<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;TTL Logic Devices, 74AC11xx and 74AC16xx Series&lt;/b&gt;&lt;p&gt;
Based on the following source:
&lt;ul&gt;
&lt;li&gt;www.ti.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SSOP48DL">
<description>&lt;B&gt;Shrink Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="SO24W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="PLCC68">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;</description>
</package>
<package name="PLCC20">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;&lt;p&gt;IPC standard</description>
</package>
<package name="PLCC28">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;&lt;p&gt;IPC standard</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="LCC28">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="2PWR1GND">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="7411000">
<pin name="I0" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="2PWR2GND">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="7411002">
<pin name="I0" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7411004">
<pin name="O" direction="out" function="dot"/>
<pin name="I" direction="in"/>
</symbol>
<symbol name="2PWR4GND">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="7411008">
<pin name="I0" direction="in"/>
<pin name="O" direction="out"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7411010">
<pin name="I0" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I2" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7411011">
<pin name="I0" direction="in"/>
<pin name="O" direction="out"/>
<pin name="I2" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7411013">
<pin name="I1" direction="in"/>
<pin name="I0" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I3" direction="in"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7411021">
<pin name="I1" direction="in"/>
<pin name="I0" direction="in"/>
<pin name="O" direction="out"/>
<pin name="I3" direction="in"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7411027">
<pin name="I0" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I2" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7411030">
<pin name="I2" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I0" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I7" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I3" direction="in"/>
</symbol>
<symbol name="7411032">
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7411034">
<pin name="O" direction="out"/>
<pin name="I" direction="in"/>
</symbol>
<symbol name="7411074">
<pin name="PR" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="CL" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="7411109">
<pin name="PR" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="CL" direction="in" function="dot"/>
<pin name="J" direction="in"/>
<pin name="K" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="7411112">
<pin name="PR" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="CL" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="K" direction="in"/>
</symbol>
<symbol name="7411138">
<pin name="Y1" direction="out" function="dot"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="Y3" direction="out" function="dot"/>
<pin name="Y4" direction="out" function="dot"/>
<pin name="Y5" direction="out" function="dot"/>
<pin name="Y6" direction="out" function="dot"/>
<pin name="Y7" direction="out" function="dot"/>
<pin name="G2B" direction="in" function="dot"/>
<pin name="G2A" direction="in" function="dot"/>
<pin name="G1" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y0" direction="out" function="dot"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="7411139">
<pin name="Y1" direction="out" function="dot"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="Y3" direction="out" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y0" direction="out" function="dot"/>
</symbol>
<symbol name="7411151">
<pin name="D0" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="Y" direction="out"/>
<pin name="W" direction="out" function="dot"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
</symbol>
<symbol name="7411153">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="1G" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2C3" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C0" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
</symbol>
<symbol name="7411157">
<pin name="!A!/B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="G" direction="in" function="dot"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
</symbol>
<symbol name="7411158">
<pin name="!A!/B" direction="in"/>
<pin name="1Y" direction="out" function="dot"/>
<pin name="2Y" direction="out" function="dot"/>
<pin name="3Y" direction="out" function="dot"/>
<pin name="4Y" direction="out" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
</symbol>
<symbol name="7411160">
<pin name="RCO" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="LOAD" direction="in" function="dot"/>
<pin name="ENT" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="7411168">
<pin name="RCO" direction="out" function="dot"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="LOAD" direction="in" function="dot"/>
<pin name="ENT" direction="in" function="dot"/>
<pin name="ENP" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="U/!D" direction="in" function="dot"/>
</symbol>
<symbol name="7411174">
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="7411175">
<pin name="!Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="!Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="!Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="!Q4" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="Q1" direction="out"/>
</symbol>
<symbol name="7411181">
<pin name="CN" direction="in"/>
<pin name="M" direction="in"/>
<pin name="A=B" direction="out"/>
<pin name="F0" direction="out" function="dot"/>
<pin name="F1" direction="out" function="dot"/>
<pin name="F2" direction="out" function="dot"/>
<pin name="F3" direction="out" function="dot"/>
<pin name="P" direction="out" function="dot"/>
<pin name="G" direction="out" function="dot"/>
<pin name="CN+4" direction="out"/>
<pin name="S3" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="B3" direction="in" function="dot"/>
<pin name="B2" direction="in" function="dot"/>
<pin name="B1" direction="in" function="dot"/>
<pin name="A3" direction="in" function="dot"/>
<pin name="A2" direction="in" function="dot"/>
<pin name="A1" direction="in" function="dot"/>
<pin name="A0" direction="in" function="dot"/>
</symbol>
<symbol name="7411190">
<pin name="RCO" direction="out" function="dot"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="MAX/MIN" direction="out"/>
<pin name="LOAD" direction="in" function="dot"/>
<pin name="CTEN" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D/!U" direction="in"/>
</symbol>
<symbol name="7411192">
<pin name="BO" direction="out" function="dot"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CO" direction="out" function="dot"/>
<pin name="LOAD" direction="in" function="dot"/>
<pin name="CLR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="UP" direction="in"/>
<pin name="DN" direction="in"/>
</symbol>
<symbol name="7411194">
<pin name="SR" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="SL" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
</symbol>
<symbol name="7411238">
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="G2B" direction="in" function="dot"/>
<pin name="G2A" direction="in" function="dot"/>
<pin name="G1" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y0" direction="out"/>
</symbol>
<symbol name="7411239">
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y0" direction="out"/>
</symbol>
<symbol name="7411240">
<pin name="Y1" direction="hiz" function="dot"/>
<pin name="Y2" direction="hiz" function="dot"/>
<pin name="Y3" direction="hiz" function="dot"/>
<pin name="Y4" direction="hiz" function="dot"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="7411241">
<pin name="2Y1" direction="hiz"/>
<pin name="2Y2" direction="hiz"/>
<pin name="2Y3" direction="hiz"/>
<pin name="2Y4" direction="hiz"/>
<pin name="2G" direction="in"/>
<pin name="2A4" direction="in"/>
<pin name="2A3" direction="in"/>
<pin name="2A2" direction="in"/>
<pin name="2A1" direction="in"/>
<pin name="1A4" direction="in"/>
<pin name="1A3" direction="in"/>
<pin name="1A2" direction="in"/>
<pin name="1A1" direction="in"/>
<pin name="1G" direction="in" function="dot"/>
</symbol>
<symbol name="7411244">
<pin name="1Y1" direction="hiz"/>
<pin name="1Y2" direction="hiz"/>
<pin name="1Y3" direction="hiz"/>
<pin name="1Y4" direction="hiz"/>
<pin name="2Y1" direction="hiz"/>
<pin name="2Y2" direction="hiz"/>
<pin name="2Y3" direction="hiz"/>
<pin name="2Y4" direction="hiz"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2A4" direction="in"/>
<pin name="2A3" direction="in"/>
<pin name="2A2" direction="in"/>
<pin name="2A1" direction="in"/>
<pin name="1A4" direction="in"/>
<pin name="1A3" direction="in"/>
<pin name="1A2" direction="in"/>
<pin name="1A1" direction="in"/>
<pin name="1G" direction="in" function="dot"/>
</symbol>
<symbol name="7411245">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="G" direction="in" function="dot"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="DIR" direction="in"/>
</symbol>
<symbol name="7411251">
<pin name="D0" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="Y" direction="hiz"/>
<pin name="W" direction="hiz" function="dot"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
</symbol>
<symbol name="7411253">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2Y" direction="hiz"/>
<pin name="1G" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2C3" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C0" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
</symbol>
<symbol name="7411257">
<pin name="!A!/B" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2Y" direction="hiz"/>
<pin name="3Y" direction="hiz"/>
<pin name="4Y" direction="hiz"/>
<pin name="G" direction="in" function="dot"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
</symbol>
<symbol name="7411258">
<pin name="!A!/B" direction="in"/>
<pin name="1Y" direction="hiz" function="dot"/>
<pin name="2Y" direction="hiz" function="dot"/>
<pin name="3Y" direction="hiz" function="dot"/>
<pin name="4Y" direction="hiz" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
</symbol>
<symbol name="7411280">
<pin name="A" direction="in"/>
<pin name="ODD" direction="out" function="dot"/>
<pin name="EVEN" direction="out"/>
<pin name="I" direction="in"/>
<pin name="H" direction="in"/>
<pin name="G" direction="in"/>
<pin name="F" direction="in"/>
<pin name="E" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
</symbol>
<symbol name="7411286">
<pin name="A" direction="in"/>
<pin name="P_I/O"/>
<pin name="P_ERR" direction="out" function="dot"/>
<pin name="XMIT" direction="in" function="dot"/>
<pin name="I" direction="in"/>
<pin name="H" direction="in"/>
<pin name="G" direction="in"/>
<pin name="F" direction="in"/>
<pin name="E" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
</symbol>
<symbol name="7411299">
<pin name="A/QA"/>
<pin name="B/QB"/>
<pin name="C/QC"/>
<pin name="D/QD"/>
<pin name="E/QE"/>
<pin name="F/QF"/>
<pin name="G/QG"/>
<pin name="H/QH"/>
<pin name="QH'" direction="out"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="SR" direction="in"/>
<pin name="SL" direction="in"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="QA'" direction="out"/>
</symbol>
<symbol name="7411352">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="1Y" direction="out" function="dot"/>
<pin name="2Y" direction="out" function="dot"/>
<pin name="1G" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2C3" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C0" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
</symbol>
<symbol name="7411353">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="1Y" direction="hiz" function="dot"/>
<pin name="2Y" direction="hiz" function="dot"/>
<pin name="1G" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2C3" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C0" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
</symbol>
<symbol name="7411373">
<pin name="Q0" direction="hiz"/>
<pin name="Q1" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q4" direction="hiz"/>
<pin name="Q5" direction="hiz"/>
<pin name="Q6" direction="hiz"/>
<pin name="Q7" direction="hiz"/>
<pin name="G" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="OC" direction="in" function="dot"/>
</symbol>
<symbol name="7411374">
<pin name="Q0" direction="hiz"/>
<pin name="Q1" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q4" direction="hiz"/>
<pin name="Q5" direction="hiz"/>
<pin name="Q6" direction="hiz"/>
<pin name="Q7" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="OC" direction="in" function="dot"/>
</symbol>
<symbol name="7411379">
<pin name="!Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="!Q2" direction="out"/>
<pin name="!Q3" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="!Q4" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="CLKEN" direction="in" function="dot"/>
<pin name="Q1" direction="out"/>
</symbol>
<symbol name="7411520">
<pin name="Q1" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P=Q" direction="out" function="dot"/>
<pin name="Q7" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="7411533">
<pin name="Q1" direction="hiz" function="dot"/>
<pin name="Q2" direction="hiz" function="dot"/>
<pin name="Q3" direction="hiz" function="dot"/>
<pin name="Q4" direction="hiz" function="dot"/>
<pin name="Q5" direction="hiz" function="dot"/>
<pin name="Q6" direction="hiz" function="dot"/>
<pin name="Q7" direction="hiz" function="dot"/>
<pin name="Q8" direction="hiz" function="dot"/>
<pin name="C" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="OE" direction="in" function="dot"/>
</symbol>
<symbol name="7411534">
<pin name="Q1" direction="hiz" function="dot"/>
<pin name="Q2" direction="hiz" function="dot"/>
<pin name="Q3" direction="hiz" function="dot"/>
<pin name="Q4" direction="hiz" function="dot"/>
<pin name="Q5" direction="hiz" function="dot"/>
<pin name="Q6" direction="hiz" function="dot"/>
<pin name="Q7" direction="hiz" function="dot"/>
<pin name="Q8" direction="hiz" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="OE" direction="in" function="dot"/>
</symbol>
<symbol name="7411620">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="GBA" direction="in" function="dot"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="GAB" direction="in"/>
</symbol>
<symbol name="7411646">
<pin name="G" direction="in" function="dot"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="DIR" direction="in"/>
<pin name="SBA" direction="in"/>
<pin name="CBA" direction="in" function="clk"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="SAB" direction="in"/>
<pin name="CAB" direction="in" function="clk"/>
</symbol>
<symbol name="7411651">
<pin name="GAB" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="GBA" direction="in" function="dot"/>
<pin name="SBA" direction="in"/>
<pin name="CBA" direction="in" function="clk"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="SAB" direction="in"/>
<pin name="CAB" direction="in" function="clk"/>
</symbol>
<symbol name="7411821">
<pin name="Q1" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q4" direction="hiz"/>
<pin name="Q5" direction="hiz"/>
<pin name="Q6" direction="hiz"/>
<pin name="Q7" direction="hiz"/>
<pin name="Q8" direction="hiz"/>
<pin name="Q9" direction="hiz"/>
<pin name="Q10" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D10" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="OC" direction="in" function="dot"/>
</symbol>
<symbol name="7411822">
<pin name="Q1" direction="hiz" function="dot"/>
<pin name="Q2" direction="hiz" function="dot"/>
<pin name="Q3" direction="hiz" function="dot"/>
<pin name="Q4" direction="hiz" function="dot"/>
<pin name="Q5" direction="hiz" function="dot"/>
<pin name="Q6" direction="hiz" function="dot"/>
<pin name="Q7" direction="hiz" function="dot"/>
<pin name="Q8" direction="hiz" function="dot"/>
<pin name="Q9" direction="hiz" function="dot"/>
<pin name="Q10" direction="hiz" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D10" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="OC" direction="in" function="dot"/>
</symbol>
<symbol name="7411823">
<pin name="Q1" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q4" direction="hiz"/>
<pin name="Q5" direction="hiz"/>
<pin name="Q6" direction="hiz"/>
<pin name="Q7" direction="hiz"/>
<pin name="Q8" direction="hiz"/>
<pin name="Q9" direction="hiz"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLKEN" direction="in" function="dot"/>
<pin name="D9" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="OC" direction="in" function="dot"/>
</symbol>
<symbol name="7411824">
<pin name="Q1" direction="hiz" function="dot"/>
<pin name="Q2" direction="hiz" function="dot"/>
<pin name="Q3" direction="hiz" function="dot"/>
<pin name="Q4" direction="hiz" function="dot"/>
<pin name="Q5" direction="hiz" function="dot"/>
<pin name="Q6" direction="hiz" function="dot"/>
<pin name="Q7" direction="hiz" function="dot"/>
<pin name="Q8" direction="hiz" function="dot"/>
<pin name="Q9" direction="hiz" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLKEN" direction="in" function="dot"/>
<pin name="D9" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="OC" direction="in" function="dot"/>
</symbol>
<symbol name="7411825">
<pin name="OC1" direction="in" function="dot"/>
<pin name="Q1" direction="hiz" function="dot"/>
<pin name="Q2" direction="hiz" function="dot"/>
<pin name="Q3" direction="hiz" function="dot"/>
<pin name="Q4" direction="hiz" function="dot"/>
<pin name="Q5" direction="hiz" function="dot"/>
<pin name="Q6" direction="hiz" function="dot"/>
<pin name="Q7" direction="hiz" function="dot"/>
<pin name="Q8" direction="hiz" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLKEN" direction="in" function="dot"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="OC3" direction="in" function="dot"/>
<pin name="OC2" direction="in" function="dot"/>
</symbol>
<symbol name="7411827">
<pin name="Y1" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y7" direction="hiz"/>
<pin name="Y8" direction="hiz"/>
<pin name="Y9" direction="hiz"/>
<pin name="Y10" direction="hiz"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="A10" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="G1" direction="in" function="dot"/>
</symbol>
<symbol name="7411833">
<pin name="PAR" function="dot"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="ERR" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="OEB" direction="in" function="dot"/>
<pin name="OEA" direction="in" function="dot"/>
</symbol>
<symbol name="7411853">
<pin name="PAR"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="ERR" function="dot"/>
<pin name="LE" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="OEB" direction="in" function="dot"/>
<pin name="OEA" direction="in" function="dot"/>
</symbol>
<symbol name="7411861">
<pin name="A1" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="A4" direction="hiz"/>
<pin name="A5" direction="hiz"/>
<pin name="A6" direction="hiz"/>
<pin name="A7" direction="hiz"/>
<pin name="A8" direction="hiz"/>
<pin name="A9" direction="hiz"/>
<pin name="A10" direction="hiz"/>
<pin name="GAB" direction="in" function="dot"/>
<pin name="B10" direction="in"/>
<pin name="B9" direction="in"/>
<pin name="B8" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="GBA" direction="in" function="dot"/>
</symbol>
<symbol name="7411882">
<pin name="G0" direction="in" function="dot"/>
<pin name="P0" direction="in" function="dot"/>
<pin name="CN" direction="in"/>
<pin name="CN+8" direction="out"/>
<pin name="CN+16" direction="out"/>
<pin name="CN+24" direction="out"/>
<pin name="CN+32" direction="out"/>
<pin name="G7" direction="in" function="dot"/>
<pin name="P7" direction="in" function="dot"/>
<pin name="G6" direction="in" function="dot"/>
<pin name="P6" direction="in" function="dot"/>
<pin name="G5" direction="in" function="dot"/>
<pin name="P5" direction="in" function="dot"/>
<pin name="G4" direction="in" function="dot"/>
<pin name="P4" direction="in" function="dot"/>
<pin name="G3" direction="in" function="dot"/>
<pin name="P3" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="P2" direction="in" function="dot"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="P1" direction="in" function="dot"/>
</symbol>
<symbol name="7411648">
<pin name="A1" function="dot"/>
<pin name="A2" function="dot"/>
<pin name="A3" function="dot"/>
<pin name="A4" function="dot"/>
<pin name="A5" function="dot"/>
<pin name="A6" function="dot"/>
<pin name="A7" function="dot"/>
<pin name="A8" function="dot"/>
<pin name="B1" function="dot"/>
<pin name="B2" function="dot"/>
<pin name="B3" function="dot"/>
<pin name="B4" function="dot"/>
<pin name="B5" function="dot"/>
<pin name="B6" function="dot"/>
<pin name="B7" function="dot"/>
<pin name="B8" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="DIR" direction="in" function="dot"/>
<pin name="CBA" direction="in" function="clk"/>
<pin name="SBA" direction="in"/>
<pin name="CAB" direction="in" function="clk"/>
<pin name="SAB" direction="in"/>
</symbol>
<symbol name="7411652">
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="G-BA" direction="in" function="dot"/>
<pin name="GAB" direction="in"/>
<pin name="CBA" direction="in" function="clk"/>
<pin name="SBA" direction="in"/>
<pin name="CAB" direction="in" function="clk"/>
<pin name="SAB" direction="in"/>
</symbol>
<symbol name="7411873">
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="Q1" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q4" direction="hiz"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="7411874">
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="Q1" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q4" direction="hiz"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="7411881">
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S3" direction="in"/>
<pin name="M" direction="in"/>
<pin name="CN" direction="in"/>
<pin name="A0" direction="in" function="dot"/>
<pin name="B0" direction="in" function="dot"/>
<pin name="A1" direction="in" function="dot"/>
<pin name="B1" direction="in" function="dot"/>
<pin name="A2" direction="in" function="dot"/>
<pin name="B2" direction="in" function="dot"/>
<pin name="A3" direction="in" function="dot"/>
<pin name="B3" direction="in" function="dot"/>
<pin name="P" direction="out" function="dot"/>
<pin name="G" direction="out" function="dot"/>
<pin name="A=B" direction="out"/>
<pin name="CN+4" direction="out"/>
<pin name="F0" direction="out" function="dot"/>
<pin name="F2" direction="out" function="dot"/>
<pin name="F1" direction="out" function="dot"/>
<pin name="F3" direction="out" function="dot"/>
</symbol>
<symbol name="7416240">
<pin name="1G" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="3G" direction="in" function="dot"/>
<pin name="4G" direction="in" function="dot"/>
<pin name="1Y1" direction="hiz" function="dot"/>
<pin name="1Y2" direction="hiz" function="dot"/>
<pin name="1Y3" direction="hiz" function="dot"/>
<pin name="1Y4" direction="hiz" function="dot"/>
<pin name="2Y1" direction="hiz" function="dot"/>
<pin name="2Y2" direction="hiz" function="dot"/>
<pin name="2Y3" direction="hiz" function="dot"/>
<pin name="2Y4" direction="hiz" function="dot"/>
<pin name="3Y1" direction="hiz" function="dot"/>
<pin name="3Y2" direction="hiz" function="dot"/>
<pin name="3Y3" direction="hiz" function="dot"/>
<pin name="3Y4" direction="hiz" function="dot"/>
<pin name="4Y1" direction="hiz" function="dot"/>
<pin name="4Y2" direction="hiz" function="dot"/>
<pin name="4Y3" direction="hiz" function="dot"/>
<pin name="4Y4" direction="hiz" function="dot"/>
<pin name="1A1" direction="in"/>
<pin name="1A2" direction="in"/>
<pin name="1A3" direction="in"/>
<pin name="1A4" direction="in"/>
<pin name="2A1" direction="in"/>
<pin name="2A2" direction="in"/>
<pin name="2A3" direction="in"/>
<pin name="2A4" direction="in"/>
<pin name="3A1" direction="in"/>
<pin name="3A2" direction="in"/>
<pin name="3A3" direction="in"/>
<pin name="3A4" direction="in"/>
<pin name="4A1" direction="in"/>
<pin name="4A2" direction="in"/>
<pin name="4A3" direction="in"/>
<pin name="4A4" direction="in"/>
</symbol>
<symbol name="7416244">
<pin name="1G" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="3G" direction="in" function="dot"/>
<pin name="4G" direction="in" function="dot"/>
<pin name="1Y1" direction="hiz"/>
<pin name="1Y2" direction="hiz"/>
<pin name="1Y3" direction="hiz"/>
<pin name="1Y4" direction="hiz"/>
<pin name="2Y1" direction="hiz"/>
<pin name="2Y2" direction="hiz"/>
<pin name="2Y3" direction="hiz"/>
<pin name="2Y4" direction="hiz"/>
<pin name="3Y1" direction="hiz"/>
<pin name="3Y2" direction="hiz"/>
<pin name="3Y3" direction="hiz"/>
<pin name="3Y4" direction="hiz"/>
<pin name="4Y1" direction="hiz"/>
<pin name="4Y2" direction="hiz"/>
<pin name="4Y3" direction="hiz"/>
<pin name="4Y4" direction="hiz"/>
<pin name="1A1" direction="in"/>
<pin name="1A2" direction="in"/>
<pin name="1A3" direction="in"/>
<pin name="1A4" direction="in"/>
<pin name="2A1" direction="in"/>
<pin name="2A2" direction="in"/>
<pin name="2A3" direction="in"/>
<pin name="2A4" direction="in"/>
<pin name="3A1" direction="in"/>
<pin name="3A2" direction="in"/>
<pin name="3A3" direction="in"/>
<pin name="3A4" direction="in"/>
<pin name="4A1" direction="in"/>
<pin name="4A2" direction="in"/>
<pin name="4A3" direction="in"/>
<pin name="4A4" direction="in"/>
</symbol>
<symbol name="7416245">
<pin name="1G" direction="in" function="dot"/>
<pin name="1DIR" direction="in" function="dot"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2DIR" direction="in" function="dot"/>
<pin name="1B1"/>
<pin name="1B2"/>
<pin name="1B3"/>
<pin name="1B4"/>
<pin name="1B5"/>
<pin name="1B6"/>
<pin name="1B7"/>
<pin name="1B8"/>
<pin name="2B1"/>
<pin name="2B2"/>
<pin name="2B3"/>
<pin name="2B4"/>
<pin name="2B5"/>
<pin name="2B6"/>
<pin name="2B7"/>
<pin name="2B8"/>
<pin name="1A1"/>
<pin name="1A2"/>
<pin name="1A3"/>
<pin name="1A4"/>
<pin name="1A5"/>
<pin name="1A6"/>
<pin name="1A7"/>
<pin name="1A8"/>
<pin name="2A1"/>
<pin name="2A2"/>
<pin name="2A3"/>
<pin name="2A4"/>
<pin name="2A5"/>
<pin name="2A6"/>
<pin name="2A7"/>
<pin name="2A8"/>
</symbol>
<symbol name="7416373">
<pin name="1OE" direction="in" function="dot"/>
<pin name="1C" direction="in"/>
<pin name="2OE" direction="in" function="dot"/>
<pin name="2C" direction="in"/>
<pin name="1Q1" direction="hiz"/>
<pin name="1Q2" direction="hiz"/>
<pin name="1Q3" direction="hiz"/>
<pin name="1Q4" direction="hiz"/>
<pin name="1Q5" direction="hiz"/>
<pin name="1Q6" direction="hiz"/>
<pin name="1Q7" direction="hiz"/>
<pin name="1Q8" direction="hiz"/>
<pin name="2Q1" direction="hiz"/>
<pin name="2Q2" direction="hiz"/>
<pin name="2Q3" direction="hiz"/>
<pin name="2Q4" direction="hiz"/>
<pin name="2Q5" direction="hiz"/>
<pin name="2Q6" direction="hiz"/>
<pin name="2Q7" direction="hiz"/>
<pin name="2Q8" direction="hiz"/>
<pin name="1D1" direction="in"/>
<pin name="1D2" direction="in"/>
<pin name="1D3" direction="in"/>
<pin name="1D4" direction="in"/>
<pin name="1D5" direction="in"/>
<pin name="1D6" direction="in"/>
<pin name="1D7" direction="in"/>
<pin name="1D8" direction="in"/>
<pin name="2D1" direction="in"/>
<pin name="2D2" direction="in"/>
<pin name="2D3" direction="in"/>
<pin name="2D4" direction="in"/>
<pin name="2D5" direction="in"/>
<pin name="2D6" direction="in"/>
<pin name="2D7" direction="in"/>
<pin name="2D8" direction="in"/>
</symbol>
<symbol name="7416374">
<pin name="1OE" direction="in" function="dot"/>
<pin name="1CLK" direction="in" function="clk"/>
<pin name="2OE" direction="in" function="dot"/>
<pin name="2CLK" direction="in" function="clk"/>
<pin name="1Q1" direction="hiz"/>
<pin name="1Q2" direction="hiz"/>
<pin name="1Q3" direction="hiz"/>
<pin name="1Q4" direction="hiz"/>
<pin name="1Q5" direction="hiz"/>
<pin name="1Q6" direction="hiz"/>
<pin name="1Q7" direction="hiz"/>
<pin name="1Q8" direction="hiz"/>
<pin name="2Q1" direction="hiz"/>
<pin name="2Q2" direction="hiz"/>
<pin name="2Q3" direction="hiz"/>
<pin name="2Q4" direction="hiz"/>
<pin name="2Q5" direction="hiz"/>
<pin name="2Q6" direction="hiz"/>
<pin name="2Q7" direction="hiz"/>
<pin name="2Q8" direction="hiz"/>
<pin name="1D1" direction="in"/>
<pin name="1D2" direction="in"/>
<pin name="1D3" direction="in"/>
<pin name="1D4" direction="in"/>
<pin name="1D5" direction="in"/>
<pin name="1D6" direction="in"/>
<pin name="1D7" direction="in"/>
<pin name="1D8" direction="in"/>
<pin name="2D1" direction="in"/>
<pin name="2D2" direction="in"/>
<pin name="2D3" direction="in"/>
<pin name="2D4" direction="in"/>
<pin name="2D5" direction="in"/>
<pin name="2D6" direction="in"/>
<pin name="2D7" direction="in"/>
<pin name="2D8" direction="in"/>
</symbol>
<symbol name="7416620">
<pin name="1GBA" direction="in" function="dot"/>
<pin name="1GAB" direction="in"/>
<pin name="2GBA" direction="in" function="dot"/>
<pin name="2GAB" direction="in"/>
<pin name="1B1"/>
<pin name="1B2"/>
<pin name="1B3"/>
<pin name="1B4"/>
<pin name="1B5"/>
<pin name="1B6"/>
<pin name="1B7"/>
<pin name="1B8"/>
<pin name="2B1"/>
<pin name="2B2"/>
<pin name="2B3"/>
<pin name="2B4"/>
<pin name="2B5"/>
<pin name="2B6"/>
<pin name="2B7"/>
<pin name="2B8"/>
<pin name="1A1"/>
<pin name="1A2"/>
<pin name="1A3"/>
<pin name="1A4"/>
<pin name="1A5"/>
<pin name="1A6"/>
<pin name="1A7"/>
<pin name="1A8"/>
<pin name="2A1"/>
<pin name="2A2"/>
<pin name="2A3"/>
<pin name="2A4"/>
<pin name="2A5"/>
<pin name="2A6"/>
<pin name="2A7"/>
<pin name="2A8"/>
</symbol>
<symbol name="4PWR8GND">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74AC11000" prefix="IC">
<description>Quadruple 2-input &lt;B&gt;NAND&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411000"/>
<gate name="B" symbol="7411000"/>
<gate name="C" symbol="7411000"/>
<gate name="D" symbol="7411000"/>
<gate name="P" symbol="2PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="15"/>
<connect gate="B" pin="I1" pad="14"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="11"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I0" pad="9"/>
<connect gate="D" pin="I1" pad="8"/>
<connect gate="D" pin="O" pad="7"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="15"/>
<connect gate="B" pin="I1" pad="14"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="11"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I0" pad="9"/>
<connect gate="D" pin="I1" pad="8"/>
<connect gate="D" pin="O" pad="7"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11002" prefix="IC">
<description>Quadruple 2-input &lt;B&gt;NOR&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411002"/>
<gate name="B" symbol="7411002"/>
<gate name="C" symbol="7411002"/>
<gate name="D" symbol="7411002"/>
<gate name="P" symbol="2PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="15"/>
<connect gate="B" pin="I1" pad="14"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="11"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I0" pad="9"/>
<connect gate="D" pin="I1" pad="8"/>
<connect gate="D" pin="O" pad="7"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="15"/>
<connect gate="B" pin="I1" pad="14"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="11"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I0" pad="9"/>
<connect gate="D" pin="I1" pad="8"/>
<connect gate="D" pin="O" pad="7"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11004" prefix="IC">
<description>Hex &lt;B&gt;INVERTER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411004"/>
<gate name="B" symbol="7411004"/>
<gate name="C" symbol="7411004"/>
<gate name="D" symbol="7411004"/>
<gate name="E" symbol="7411004"/>
<gate name="F" symbol="7411004"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="I" pad="20"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I" pad="19"/>
<connect gate="B" pin="O" pad="2"/>
<connect gate="C" pin="I" pad="18"/>
<connect gate="C" pin="O" pad="3"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="12"/>
<connect gate="E" pin="O" pad="9"/>
<connect gate="F" pin="I" pad="11"/>
<connect gate="F" pin="O" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="I" pad="20"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I" pad="19"/>
<connect gate="B" pin="O" pad="2"/>
<connect gate="C" pin="I" pad="18"/>
<connect gate="C" pin="O" pad="3"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="12"/>
<connect gate="E" pin="O" pad="9"/>
<connect gate="F" pin="I" pad="11"/>
<connect gate="F" pin="O" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11008" prefix="IC">
<description>Quadruple 2-input &lt;B&gt;AND&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411008"/>
<gate name="B" symbol="7411008"/>
<gate name="C" symbol="7411008"/>
<gate name="D" symbol="7411008"/>
<gate name="P" symbol="2PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="15"/>
<connect gate="B" pin="I1" pad="14"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="11"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I0" pad="9"/>
<connect gate="D" pin="I1" pad="8"/>
<connect gate="D" pin="O" pad="7"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="15"/>
<connect gate="B" pin="I1" pad="14"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="11"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I0" pad="9"/>
<connect gate="D" pin="I1" pad="8"/>
<connect gate="D" pin="O" pad="7"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11010" prefix="IC">
<description>Triple 3-input &lt;B&gt;NAND&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411010"/>
<gate name="B" symbol="7411010"/>
<gate name="C" symbol="7411010"/>
<gate name="P" symbol="2PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I2" pad="15"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="14"/>
<connect gate="B" pin="I1" pad="11"/>
<connect gate="B" pin="I2" pad="10"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="I2" pad="7"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I2" pad="15"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="14"/>
<connect gate="B" pin="I1" pad="11"/>
<connect gate="B" pin="I2" pad="10"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="I2" pad="7"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11011" prefix="IC">
<description>Triple 3-input &lt;B&gt;AND&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411011"/>
<gate name="B" symbol="7411010"/>
<gate name="C" symbol="7411010"/>
<gate name="P" symbol="2PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I2" pad="15"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="14"/>
<connect gate="B" pin="I1" pad="11"/>
<connect gate="B" pin="I2" pad="10"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="I2" pad="7"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I2" pad="15"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="14"/>
<connect gate="B" pin="I1" pad="11"/>
<connect gate="B" pin="I2" pad="10"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="I2" pad="7"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11013" prefix="IC">
<description>Dual 4-input &lt;B&gt;NAND&lt;/B&gt;, schmitt trigger</description>
<gates>
<gate name="A" symbol="7411013"/>
<gate name="B" symbol="7411013"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="1"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="I3" pad="12"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="10"/>
<connect gate="B" pin="I1" pad="9"/>
<connect gate="B" pin="I2" pad="7"/>
<connect gate="B" pin="I3" pad="6"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="1"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="I3" pad="12"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="10"/>
<connect gate="B" pin="I1" pad="9"/>
<connect gate="B" pin="I2" pad="7"/>
<connect gate="B" pin="I3" pad="6"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11021" prefix="IC">
<description>Dual 4-input &lt;B&gt;AND&lt;/B&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="A" symbol="7411021"/>
<gate name="B" symbol="7411021"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="1"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="I3" pad="12"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="10"/>
<connect gate="B" pin="I1" pad="9"/>
<connect gate="B" pin="I2" pad="7"/>
<connect gate="B" pin="I3" pad="6"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="1"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="I3" pad="12"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="10"/>
<connect gate="B" pin="I1" pad="9"/>
<connect gate="B" pin="I2" pad="7"/>
<connect gate="B" pin="I3" pad="6"/>
<connect gate="B" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11027" prefix="IC">
<description>Triple 3-input &lt;B&gt;NOR&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411027"/>
<gate name="B" symbol="7411027"/>
<gate name="C" symbol="7411027"/>
<gate name="P" symbol="2PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I2" pad="15"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="14"/>
<connect gate="B" pin="I1" pad="11"/>
<connect gate="B" pin="I2" pad="10"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="I2" pad="7"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I2" pad="15"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="14"/>
<connect gate="B" pin="I1" pad="11"/>
<connect gate="B" pin="I2" pad="10"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="I2" pad="7"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11030" prefix="IC">
<description>8-input &lt;B&gt;NAND&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411030"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="3"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="1"/>
<connect gate="A" pin="I3" pad="14"/>
<connect gate="A" pin="I4" pad="13"/>
<connect gate="A" pin="I5" pad="12"/>
<connect gate="A" pin="I6" pad="9"/>
<connect gate="A" pin="I7" pad="8"/>
<connect gate="A" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="3"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="1"/>
<connect gate="A" pin="I3" pad="14"/>
<connect gate="A" pin="I4" pad="13"/>
<connect gate="A" pin="I5" pad="12"/>
<connect gate="A" pin="I6" pad="9"/>
<connect gate="A" pin="I7" pad="8"/>
<connect gate="A" pin="O" pad="5"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11032" prefix="IC">
<description>Quadruple 2-input &lt;B&gt;OR&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411032"/>
<gate name="B" symbol="7411032"/>
<gate name="C" symbol="7411032"/>
<gate name="D" symbol="7411032"/>
<gate name="P" symbol="2PWR2GND"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="I1" pad="1"/>
<connect gate="A" pin="I2" pad="16"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I1" pad="15"/>
<connect gate="B" pin="I2" pad="14"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I1" pad="11"/>
<connect gate="C" pin="I2" pad="10"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I1" pad="9"/>
<connect gate="D" pin="I2" pad="8"/>
<connect gate="D" pin="O" pad="7"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="I1" pad="1"/>
<connect gate="A" pin="I2" pad="16"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I1" pad="15"/>
<connect gate="B" pin="I2" pad="14"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I1" pad="11"/>
<connect gate="C" pin="I2" pad="10"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I1" pad="9"/>
<connect gate="D" pin="I2" pad="8"/>
<connect gate="D" pin="O" pad="7"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11034" prefix="IC">
<description>Hex non-inverting &lt;B&gt;DRIVER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411034"/>
<gate name="B" symbol="7411034"/>
<gate name="C" symbol="7411034"/>
<gate name="D" symbol="7411034"/>
<gate name="E" symbol="7411034"/>
<gate name="F" symbol="7411034"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="I" pad="20"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I" pad="19"/>
<connect gate="B" pin="O" pad="2"/>
<connect gate="C" pin="I" pad="18"/>
<connect gate="C" pin="O" pad="3"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="12"/>
<connect gate="E" pin="O" pad="9"/>
<connect gate="F" pin="I" pad="11"/>
<connect gate="F" pin="O" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="I" pad="20"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I" pad="19"/>
<connect gate="B" pin="O" pad="2"/>
<connect gate="C" pin="I" pad="18"/>
<connect gate="C" pin="O" pad="3"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="12"/>
<connect gate="E" pin="O" pad="9"/>
<connect gate="F" pin="I" pad="11"/>
<connect gate="F" pin="O" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11074" prefix="IC">
<description>Dual positive edge triggered D-type &lt;B&gt;FLIP FLOP&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411074"/>
<gate name="B" symbol="7411074"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="3"/>
<connect gate="A" pin="CL" pad="12"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="PR" pad="1"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="B" pin="!Q" pad="5"/>
<connect gate="B" pin="CL" pad="10"/>
<connect gate="B" pin="CLK" pad="8"/>
<connect gate="B" pin="D" pad="9"/>
<connect gate="B" pin="PR" pad="7"/>
<connect gate="B" pin="Q" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="!Q" pad="3"/>
<connect gate="A" pin="CL" pad="12"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="PR" pad="1"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="B" pin="!Q" pad="5"/>
<connect gate="B" pin="CL" pad="10"/>
<connect gate="B" pin="CLK" pad="8"/>
<connect gate="B" pin="D" pad="9"/>
<connect gate="B" pin="PR" pad="7"/>
<connect gate="B" pin="Q" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11109" prefix="IC">
<description>Dual J-K positive edge triggered &lt;B&gt;FLIP FLOP&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411109"/>
<gate name="B" symbol="7411109"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="!Q" pad="3"/>
<connect gate="A" pin="CL" pad="13"/>
<connect gate="A" pin="CLK" pad="16"/>
<connect gate="A" pin="J" pad="14"/>
<connect gate="A" pin="K" pad="15"/>
<connect gate="A" pin="PR" pad="1"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="B" pin="!Q" pad="5"/>
<connect gate="B" pin="CL" pad="11"/>
<connect gate="B" pin="CLK" pad="8"/>
<connect gate="B" pin="J" pad="10"/>
<connect gate="B" pin="K" pad="9"/>
<connect gate="B" pin="PR" pad="7"/>
<connect gate="B" pin="Q" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q" pad="3"/>
<connect gate="A" pin="CL" pad="13"/>
<connect gate="A" pin="CLK" pad="16"/>
<connect gate="A" pin="J" pad="14"/>
<connect gate="A" pin="K" pad="15"/>
<connect gate="A" pin="PR" pad="1"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="B" pin="!Q" pad="5"/>
<connect gate="B" pin="CL" pad="11"/>
<connect gate="B" pin="CLK" pad="8"/>
<connect gate="B" pin="J" pad="10"/>
<connect gate="B" pin="K" pad="9"/>
<connect gate="B" pin="PR" pad="7"/>
<connect gate="B" pin="Q" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11112" prefix="IC">
<description>Dual J-K negative edge triggered &lt;B&gt;FLIP FLOP&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411112"/>
<gate name="B" symbol="7411112"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="!Q" pad="3"/>
<connect gate="A" pin="CL" pad="13"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="K" pad="16"/>
<connect gate="A" pin="PR" pad="1"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="B" pin="!Q" pad="5"/>
<connect gate="B" pin="CL" pad="11"/>
<connect gate="B" pin="CLK" pad="10"/>
<connect gate="B" pin="K" pad="9"/>
<connect gate="B" pin="PR" pad="7"/>
<connect gate="B" pin="Q" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q" pad="3"/>
<connect gate="A" pin="CL" pad="13"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="K" pad="16"/>
<connect gate="A" pin="PR" pad="1"/>
<connect gate="A" pin="Q" pad="2"/>
<connect gate="B" pin="!Q" pad="5"/>
<connect gate="B" pin="CL" pad="11"/>
<connect gate="B" pin="CLK" pad="10"/>
<connect gate="B" pin="K" pad="9"/>
<connect gate="B" pin="PR" pad="7"/>
<connect gate="B" pin="Q" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11138" prefix="IC">
<description>3 to 8 line &lt;B&gt;DECODER/DEMULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411138"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="G1" pad="11"/>
<connect gate="A" pin="G2A" pad="10"/>
<connect gate="A" pin="G2B" pad="9"/>
<connect gate="A" pin="Y0" pad="16"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="5"/>
<connect gate="A" pin="Y5" pad="6"/>
<connect gate="A" pin="Y6" pad="7"/>
<connect gate="A" pin="Y7" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="G1" pad="11"/>
<connect gate="A" pin="G2A" pad="10"/>
<connect gate="A" pin="G2B" pad="9"/>
<connect gate="A" pin="Y0" pad="16"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="5"/>
<connect gate="A" pin="Y5" pad="6"/>
<connect gate="A" pin="Y6" pad="7"/>
<connect gate="A" pin="Y7" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11139" prefix="IC">
<description>Dual 2 to 4 line &lt;B&gt;DECODER/DEMULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411139"/>
<gate name="B" symbol="7411139"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="Y0" pad="16"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="B" pin="A" pad="10"/>
<connect gate="B" pin="B" pad="9"/>
<connect gate="B" pin="G" pad="11"/>
<connect gate="B" pin="Y0" pad="5"/>
<connect gate="B" pin="Y1" pad="6"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="Y0" pad="16"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="B" pin="A" pad="10"/>
<connect gate="B" pin="B" pad="9"/>
<connect gate="B" pin="G" pad="11"/>
<connect gate="B" pin="Y0" pad="5"/>
<connect gate="B" pin="Y1" pad="6"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11151" prefix="IC">
<description>1 of 8 &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411151"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="C" pad="8"/>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="16"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="11"/>
<connect gate="A" pin="D6" pad="10"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="G" pad="2"/>
<connect gate="A" pin="W" pad="5"/>
<connect gate="A" pin="Y" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="C" pad="8"/>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="16"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="11"/>
<connect gate="A" pin="D6" pad="10"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="G" pad="2"/>
<connect gate="A" pin="W" pad="5"/>
<connect gate="A" pin="Y" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11153" prefix="IC">
<description>Dual 1 of 4 &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411153"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="1C0" pad="16"/>
<connect gate="A" pin="1C1" pad="15"/>
<connect gate="A" pin="1C2" pad="14"/>
<connect gate="A" pin="1C3" pad="13"/>
<connect gate="A" pin="1G" pad="6"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2C0" pad="11"/>
<connect gate="A" pin="2C1" pad="10"/>
<connect gate="A" pin="2C2" pad="9"/>
<connect gate="A" pin="2C3" pad="8"/>
<connect gate="A" pin="2G" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C0" pad="16"/>
<connect gate="A" pin="1C1" pad="15"/>
<connect gate="A" pin="1C2" pad="14"/>
<connect gate="A" pin="1C3" pad="13"/>
<connect gate="A" pin="1G" pad="6"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2C0" pad="11"/>
<connect gate="A" pin="2C1" pad="10"/>
<connect gate="A" pin="2C2" pad="9"/>
<connect gate="A" pin="2C3" pad="8"/>
<connect gate="A" pin="2G" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11157" prefix="IC">
<description>Quadruple 2 to 1 line &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411157"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="20"/>
<connect gate="A" pin="1B" pad="19"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="2A" pad="18"/>
<connect gate="A" pin="2B" pad="17"/>
<connect gate="A" pin="2Y" pad="3"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="8"/>
<connect gate="A" pin="4A" pad="12"/>
<connect gate="A" pin="4B" pad="11"/>
<connect gate="A" pin="4Y" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="20"/>
<connect gate="A" pin="1B" pad="19"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="2A" pad="18"/>
<connect gate="A" pin="2B" pad="17"/>
<connect gate="A" pin="2Y" pad="3"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="8"/>
<connect gate="A" pin="4A" pad="12"/>
<connect gate="A" pin="4B" pad="11"/>
<connect gate="A" pin="4Y" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11158" prefix="IC">
<description>Quadruple 2 to 1 line &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411158"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="20"/>
<connect gate="A" pin="1B" pad="19"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="2A" pad="18"/>
<connect gate="A" pin="2B" pad="17"/>
<connect gate="A" pin="2Y" pad="3"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="8"/>
<connect gate="A" pin="4A" pad="12"/>
<connect gate="A" pin="4B" pad="11"/>
<connect gate="A" pin="4Y" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="20"/>
<connect gate="A" pin="1B" pad="19"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="2A" pad="18"/>
<connect gate="A" pin="2B" pad="17"/>
<connect gate="A" pin="2Y" pad="3"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="8"/>
<connect gate="A" pin="4A" pad="12"/>
<connect gate="A" pin="4B" pad="11"/>
<connect gate="A" pin="4Y" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11160" prefix="IC">
<description>Synchronous 4-bit decade &lt;B&gt;Counter&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411160"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="17"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLK" pad="19"/>
<connect gate="A" pin="CLR" pad="20"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="ENP" pad="12"/>
<connect gate="A" pin="ENT" pad="11"/>
<connect gate="A" pin="LOAD" pad="10"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="3"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="RCO" pad="1"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="17"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLK" pad="19"/>
<connect gate="A" pin="CLR" pad="20"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="ENP" pad="12"/>
<connect gate="A" pin="ENT" pad="11"/>
<connect gate="A" pin="LOAD" pad="10"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="3"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="RCO" pad="1"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11174" prefix="IC">
<description>6-bit positive edge triggered D-type &lt;B&gt;FLIP FLOP&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411174"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="20"/>
<connect gate="A" pin="D1" pad="19"/>
<connect gate="A" pin="D2" pad="18"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="14"/>
<connect gate="A" pin="D5" pad="13"/>
<connect gate="A" pin="D6" pad="12"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="8"/>
<connect gate="A" pin="Q5" pad="9"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="20"/>
<connect gate="A" pin="D1" pad="19"/>
<connect gate="A" pin="D2" pad="18"/>
<connect gate="A" pin="D3" pad="17"/>
<connect gate="A" pin="D4" pad="14"/>
<connect gate="A" pin="D5" pad="13"/>
<connect gate="A" pin="D6" pad="12"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="8"/>
<connect gate="A" pin="Q5" pad="9"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11175" prefix="IC">
<description>Quadruple positive edge triggered D-type &lt;B&gt;Flip-Flop&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411175"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="!Q1" pad="1"/>
<connect gate="A" pin="!Q2" pad="3"/>
<connect gate="A" pin="!Q3" pad="9"/>
<connect gate="A" pin="!Q4" pad="11"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="19"/>
<connect gate="A" pin="D1" pad="18"/>
<connect gate="A" pin="D2" pad="17"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="Q1" pad="20"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="8"/>
<connect gate="A" pin="Q4" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="!Q1" pad="1"/>
<connect gate="A" pin="!Q2" pad="3"/>
<connect gate="A" pin="!Q3" pad="9"/>
<connect gate="A" pin="!Q4" pad="11"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="19"/>
<connect gate="A" pin="D1" pad="18"/>
<connect gate="A" pin="D2" pad="17"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="Q1" pad="20"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="8"/>
<connect gate="A" pin="Q4" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11181" prefix="IC">
<description>&lt;B&gt;ALU/FUNCTION GENERATOR&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411181"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="A0" pad="28"/>
<connect gate="A" pin="A1" pad="27"/>
<connect gate="A" pin="A2" pad="26"/>
<connect gate="A" pin="A3" pad="25"/>
<connect gate="A" pin="A=B" pad="3"/>
<connect gate="A" pin="B1" pad="23"/>
<connect gate="A" pin="B2" pad="20"/>
<connect gate="A" pin="B3" pad="19"/>
<connect gate="A" pin="CN" pad="1"/>
<connect gate="A" pin="CN+4" pad="14"/>
<connect gate="A" pin="F0" pad="4"/>
<connect gate="A" pin="F1" pad="5"/>
<connect gate="A" pin="F2" pad="10"/>
<connect gate="A" pin="F3" pad="11"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="M" pad="2"/>
<connect gate="A" pin="P" pad="12"/>
<connect gate="A" pin="S0" pad="18"/>
<connect gate="A" pin="S1" pad="17"/>
<connect gate="A" pin="S2" pad="16"/>
<connect gate="A" pin="S3" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="A0" pad="28"/>
<connect gate="A" pin="A1" pad="27"/>
<connect gate="A" pin="A2" pad="26"/>
<connect gate="A" pin="A3" pad="25"/>
<connect gate="A" pin="A=B" pad="3"/>
<connect gate="A" pin="B1" pad="23"/>
<connect gate="A" pin="B2" pad="20"/>
<connect gate="A" pin="B3" pad="19"/>
<connect gate="A" pin="CN" pad="1"/>
<connect gate="A" pin="CN+4" pad="14"/>
<connect gate="A" pin="F0" pad="4"/>
<connect gate="A" pin="F1" pad="5"/>
<connect gate="A" pin="F2" pad="10"/>
<connect gate="A" pin="F3" pad="11"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="M" pad="2"/>
<connect gate="A" pin="P" pad="12"/>
<connect gate="A" pin="S0" pad="18"/>
<connect gate="A" pin="S1" pad="17"/>
<connect gate="A" pin="S2" pad="16"/>
<connect gate="A" pin="S3" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11190" prefix="IC">
<description>Synchronous 4-bit up down decade &lt;B&gt;COUNTER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411190"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="17"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLK" pad="19"/>
<connect gate="A" pin="CTEN" pad="12"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="D/!U" pad="20"/>
<connect gate="A" pin="LOAD" pad="11"/>
<connect gate="A" pin="MAX/MIN" pad="10"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="3"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="RCO" pad="1"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="17"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLK" pad="19"/>
<connect gate="A" pin="CTEN" pad="12"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="D/!U" pad="20"/>
<connect gate="A" pin="LOAD" pad="11"/>
<connect gate="A" pin="MAX/MIN" pad="10"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="3"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="RCO" pad="1"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11192" prefix="IC">
<description>Up down &lt;B&gt;COUNTER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411192"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="17"/>
<connect gate="A" pin="BO" pad="1"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLR" pad="12"/>
<connect gate="A" pin="CO" pad="10"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="DN" pad="20"/>
<connect gate="A" pin="LOAD" pad="11"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="3"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="UP" pad="19"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="17"/>
<connect gate="A" pin="BO" pad="1"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLR" pad="12"/>
<connect gate="A" pin="CO" pad="10"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="DN" pad="20"/>
<connect gate="A" pin="LOAD" pad="11"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="3"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="UP" pad="19"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11194" prefix="IC">
<description>4-bit bidirectional universal &lt;B&gt;SHIFT REGISTER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411194"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="17"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="12"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="3"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="S0" pad="20"/>
<connect gate="A" pin="S1" pad="19"/>
<connect gate="A" pin="SL" pad="10"/>
<connect gate="A" pin="SR" pad="1"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="17"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="12"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="3"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="S0" pad="20"/>
<connect gate="A" pin="S1" pad="19"/>
<connect gate="A" pin="SL" pad="10"/>
<connect gate="A" pin="SR" pad="1"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11238" prefix="IC">
<description>3 to 8 line &lt;B&gt;DECODER/DEMULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411238"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="G1" pad="11"/>
<connect gate="A" pin="G2A" pad="10"/>
<connect gate="A" pin="G2B" pad="9"/>
<connect gate="A" pin="Y0" pad="16"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="5"/>
<connect gate="A" pin="Y5" pad="6"/>
<connect gate="A" pin="Y6" pad="7"/>
<connect gate="A" pin="Y7" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="G1" pad="11"/>
<connect gate="A" pin="G2A" pad="10"/>
<connect gate="A" pin="G2B" pad="9"/>
<connect gate="A" pin="Y0" pad="16"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="5"/>
<connect gate="A" pin="Y5" pad="6"/>
<connect gate="A" pin="Y6" pad="7"/>
<connect gate="A" pin="Y7" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11239" prefix="IC">
<description>Dual 2 to 4 line &lt;B&gt;DECODER/DEMULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411239"/>
<gate name="B" symbol="7411239"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="Y0" pad="16"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="B" pin="A" pad="10"/>
<connect gate="B" pin="B" pad="9"/>
<connect gate="B" pin="G" pad="11"/>
<connect gate="B" pin="Y0" pad="5"/>
<connect gate="B" pin="Y1" pad="6"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="Y0" pad="16"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="B" pin="A" pad="10"/>
<connect gate="B" pin="B" pad="9"/>
<connect gate="B" pin="G" pad="11"/>
<connect gate="B" pin="Y0" pad="5"/>
<connect gate="B" pin="Y1" pad="6"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11240" prefix="IC">
<description>Octal &lt;B&gt;BUFFER/DRIVER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411240"/>
<gate name="B" symbol="7411240"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="A1" pad="23"/>
<connect gate="A" pin="A2" pad="22"/>
<connect gate="A" pin="A3" pad="21"/>
<connect gate="A" pin="A4" pad="20"/>
<connect gate="A" pin="G" pad="24"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="4"/>
<connect gate="B" pin="A1" pad="17"/>
<connect gate="B" pin="A2" pad="16"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="14"/>
<connect gate="B" pin="G" pad="13"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="10"/>
<connect gate="B" pin="Y3" pad="11"/>
<connect gate="B" pin="Y4" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="A1" pad="23"/>
<connect gate="A" pin="A2" pad="22"/>
<connect gate="A" pin="A3" pad="21"/>
<connect gate="A" pin="A4" pad="20"/>
<connect gate="A" pin="G" pad="24"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="4"/>
<connect gate="B" pin="A1" pad="17"/>
<connect gate="B" pin="A2" pad="16"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="14"/>
<connect gate="B" pin="G" pad="13"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="10"/>
<connect gate="B" pin="Y3" pad="11"/>
<connect gate="B" pin="Y4" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11241" prefix="IC">
<description>Octal &lt;B&gt;BUFFER/DRIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411241"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="1A1" pad="23"/>
<connect gate="A" pin="1A2" pad="22"/>
<connect gate="A" pin="1A3" pad="21"/>
<connect gate="A" pin="1A4" pad="20"/>
<connect gate="A" pin="1G" pad="24"/>
<connect gate="A" pin="2A1" pad="17"/>
<connect gate="A" pin="2A2" pad="16"/>
<connect gate="A" pin="2A3" pad="15"/>
<connect gate="A" pin="2A4" pad="14"/>
<connect gate="A" pin="2G" pad="13"/>
<connect gate="A" pin="2Y1" pad="9"/>
<connect gate="A" pin="2Y2" pad="10"/>
<connect gate="A" pin="2Y3" pad="11"/>
<connect gate="A" pin="2Y4" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="1A1" pad="23"/>
<connect gate="A" pin="1A2" pad="22"/>
<connect gate="A" pin="1A3" pad="21"/>
<connect gate="A" pin="1A4" pad="20"/>
<connect gate="A" pin="1G" pad="24"/>
<connect gate="A" pin="2A1" pad="17"/>
<connect gate="A" pin="2A2" pad="16"/>
<connect gate="A" pin="2A3" pad="15"/>
<connect gate="A" pin="2A4" pad="14"/>
<connect gate="A" pin="2G" pad="13"/>
<connect gate="A" pin="2Y1" pad="9"/>
<connect gate="A" pin="2Y2" pad="10"/>
<connect gate="A" pin="2Y3" pad="11"/>
<connect gate="A" pin="2Y4" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11244" prefix="IC">
<description>Octal &lt;B&gt;BUFFER/DRIVER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411244"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="1A1" pad="23"/>
<connect gate="A" pin="1A2" pad="22"/>
<connect gate="A" pin="1A3" pad="21"/>
<connect gate="A" pin="1A4" pad="20"/>
<connect gate="A" pin="1G" pad="24"/>
<connect gate="A" pin="1Y1" pad="1"/>
<connect gate="A" pin="1Y2" pad="2"/>
<connect gate="A" pin="1Y3" pad="3"/>
<connect gate="A" pin="1Y4" pad="4"/>
<connect gate="A" pin="2A1" pad="17"/>
<connect gate="A" pin="2A2" pad="16"/>
<connect gate="A" pin="2A3" pad="15"/>
<connect gate="A" pin="2A4" pad="14"/>
<connect gate="A" pin="2G" pad="13"/>
<connect gate="A" pin="2Y1" pad="9"/>
<connect gate="A" pin="2Y2" pad="10"/>
<connect gate="A" pin="2Y3" pad="11"/>
<connect gate="A" pin="2Y4" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="1A1" pad="23"/>
<connect gate="A" pin="1A2" pad="22"/>
<connect gate="A" pin="1A3" pad="21"/>
<connect gate="A" pin="1A4" pad="20"/>
<connect gate="A" pin="1G" pad="24"/>
<connect gate="A" pin="1Y1" pad="1"/>
<connect gate="A" pin="1Y2" pad="2"/>
<connect gate="A" pin="1Y3" pad="3"/>
<connect gate="A" pin="1Y4" pad="4"/>
<connect gate="A" pin="2A1" pad="17"/>
<connect gate="A" pin="2A2" pad="16"/>
<connect gate="A" pin="2A3" pad="15"/>
<connect gate="A" pin="2A4" pad="14"/>
<connect gate="A" pin="2G" pad="13"/>
<connect gate="A" pin="2Y1" pad="9"/>
<connect gate="A" pin="2Y2" pad="10"/>
<connect gate="A" pin="2Y3" pad="11"/>
<connect gate="A" pin="2Y4" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11245" prefix="IC">
<description>Octal &lt;B&gt;BUS TRANSCEIVER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411245"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="9"/>
<connect gate="A" pin="A6" pad="10"/>
<connect gate="A" pin="A7" pad="11"/>
<connect gate="A" pin="A8" pad="12"/>
<connect gate="A" pin="B1" pad="23"/>
<connect gate="A" pin="B2" pad="22"/>
<connect gate="A" pin="B3" pad="21"/>
<connect gate="A" pin="B4" pad="20"/>
<connect gate="A" pin="B5" pad="17"/>
<connect gate="A" pin="B6" pad="16"/>
<connect gate="A" pin="B7" pad="15"/>
<connect gate="A" pin="B8" pad="14"/>
<connect gate="A" pin="DIR" pad="24"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="9"/>
<connect gate="A" pin="A6" pad="10"/>
<connect gate="A" pin="A7" pad="11"/>
<connect gate="A" pin="A8" pad="12"/>
<connect gate="A" pin="B1" pad="23"/>
<connect gate="A" pin="B2" pad="22"/>
<connect gate="A" pin="B3" pad="21"/>
<connect gate="A" pin="B4" pad="20"/>
<connect gate="A" pin="B5" pad="17"/>
<connect gate="A" pin="B6" pad="16"/>
<connect gate="A" pin="B7" pad="15"/>
<connect gate="A" pin="B8" pad="14"/>
<connect gate="A" pin="DIR" pad="24"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11251" prefix="IC">
<description>1 of 8 &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411251"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="C" pad="8"/>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="16"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="11"/>
<connect gate="A" pin="D6" pad="10"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="G" pad="2"/>
<connect gate="A" pin="W" pad="5"/>
<connect gate="A" pin="Y" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="6"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="C" pad="8"/>
<connect gate="A" pin="D0" pad="1"/>
<connect gate="A" pin="D1" pad="16"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="11"/>
<connect gate="A" pin="D6" pad="10"/>
<connect gate="A" pin="D7" pad="9"/>
<connect gate="A" pin="G" pad="2"/>
<connect gate="A" pin="W" pad="5"/>
<connect gate="A" pin="Y" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11253" prefix="IC">
<description>Dual 4 to 1 line &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411253"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="1C0" pad="16"/>
<connect gate="A" pin="1C1" pad="15"/>
<connect gate="A" pin="1C2" pad="14"/>
<connect gate="A" pin="1C3" pad="13"/>
<connect gate="A" pin="1G" pad="6"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2C0" pad="11"/>
<connect gate="A" pin="2C1" pad="10"/>
<connect gate="A" pin="2C2" pad="9"/>
<connect gate="A" pin="2C3" pad="8"/>
<connect gate="A" pin="2G" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C0" pad="16"/>
<connect gate="A" pin="1C1" pad="15"/>
<connect gate="A" pin="1C2" pad="14"/>
<connect gate="A" pin="1C3" pad="13"/>
<connect gate="A" pin="1G" pad="6"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2C0" pad="11"/>
<connect gate="A" pin="2C1" pad="10"/>
<connect gate="A" pin="2C2" pad="9"/>
<connect gate="A" pin="2C3" pad="8"/>
<connect gate="A" pin="2G" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11257" prefix="IC">
<description>Quadruple 2 to 1 line &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411257"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="20"/>
<connect gate="A" pin="1B" pad="19"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="2A" pad="18"/>
<connect gate="A" pin="2B" pad="17"/>
<connect gate="A" pin="2Y" pad="3"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="8"/>
<connect gate="A" pin="4A" pad="12"/>
<connect gate="A" pin="4B" pad="11"/>
<connect gate="A" pin="4Y" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="20"/>
<connect gate="A" pin="1B" pad="19"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="2A" pad="18"/>
<connect gate="A" pin="2B" pad="17"/>
<connect gate="A" pin="2Y" pad="3"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="8"/>
<connect gate="A" pin="4A" pad="12"/>
<connect gate="A" pin="4B" pad="11"/>
<connect gate="A" pin="4Y" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11258" prefix="IC">
<description>Quadruple 2 to 1 line &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411258"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="20"/>
<connect gate="A" pin="1B" pad="19"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="2A" pad="18"/>
<connect gate="A" pin="2B" pad="17"/>
<connect gate="A" pin="2Y" pad="3"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="8"/>
<connect gate="A" pin="4A" pad="12"/>
<connect gate="A" pin="4B" pad="11"/>
<connect gate="A" pin="4Y" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="20"/>
<connect gate="A" pin="1B" pad="19"/>
<connect gate="A" pin="1Y" pad="2"/>
<connect gate="A" pin="2A" pad="18"/>
<connect gate="A" pin="2B" pad="17"/>
<connect gate="A" pin="2Y" pad="3"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="8"/>
<connect gate="A" pin="4A" pad="12"/>
<connect gate="A" pin="4B" pad="11"/>
<connect gate="A" pin="4Y" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11280" prefix="IC">
<description>9-bit &lt;B&gt;PARITY GENERATOR/CHECKER&lt;/B&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="P1" symbol="7411280"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
<connect gate="P1" pin="A" pad="2"/>
<connect gate="P1" pin="B" pad="1"/>
<connect gate="P1" pin="C" pad="14"/>
<connect gate="P1" pin="D" pad="13"/>
<connect gate="P1" pin="E" pad="12"/>
<connect gate="P1" pin="EVEN" pad="5"/>
<connect gate="P1" pin="F" pad="10"/>
<connect gate="P1" pin="G" pad="9"/>
<connect gate="P1" pin="H" pad="8"/>
<connect gate="P1" pin="I" pad="7"/>
<connect gate="P1" pin="ODD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
<connect gate="P1" pin="A" pad="2"/>
<connect gate="P1" pin="B" pad="1"/>
<connect gate="P1" pin="C" pad="14"/>
<connect gate="P1" pin="D" pad="13"/>
<connect gate="P1" pin="E" pad="12"/>
<connect gate="P1" pin="EVEN" pad="5"/>
<connect gate="P1" pin="F" pad="10"/>
<connect gate="P1" pin="G" pad="9"/>
<connect gate="P1" pin="H" pad="8"/>
<connect gate="P1" pin="I" pad="7"/>
<connect gate="P1" pin="ODD" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11286" prefix="IC">
<description>9-bit &lt;B&gt;PARITY GENERATOR/CHECKER&lt;/B&gt;, bus driver</description>
<gates>
<gate name="A" symbol="7411286"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="E" pad="12"/>
<connect gate="A" pin="F" pad="10"/>
<connect gate="A" pin="G" pad="9"/>
<connect gate="A" pin="H" pad="8"/>
<connect gate="A" pin="I" pad="7"/>
<connect gate="A" pin="P_ERR" pad="5"/>
<connect gate="A" pin="P_I/O" pad="3"/>
<connect gate="A" pin="XMIT" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="E" pad="12"/>
<connect gate="A" pin="F" pad="10"/>
<connect gate="A" pin="G" pad="9"/>
<connect gate="A" pin="H" pad="8"/>
<connect gate="A" pin="I" pad="7"/>
<connect gate="A" pin="P_ERR" pad="5"/>
<connect gate="A" pin="P_I/O" pad="3"/>
<connect gate="A" pin="XMIT" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11299" prefix="IC">
<description>8-bit universal &lt;B&gt;SHIFT/STORAGE REGISTER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411299"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="A/QA" pad="1"/>
<connect gate="A" pin="B/QB" pad="2"/>
<connect gate="A" pin="C/QC" pad="3"/>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D/QD" pad="4"/>
<connect gate="A" pin="E/QE" pad="9"/>
<connect gate="A" pin="F/QF" pad="10"/>
<connect gate="A" pin="G/QG" pad="11"/>
<connect gate="A" pin="G1" pad="21"/>
<connect gate="A" pin="G2" pad="20"/>
<connect gate="A" pin="H/QH" pad="12"/>
<connect gate="A" pin="QA'" pad="24"/>
<connect gate="A" pin="QH'" pad="13"/>
<connect gate="A" pin="S0" pad="23"/>
<connect gate="A" pin="S1" pad="22"/>
<connect gate="A" pin="SL" pad="17"/>
<connect gate="A" pin="SR" pad="16"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="A/QA" pad="1"/>
<connect gate="A" pin="B/QB" pad="2"/>
<connect gate="A" pin="C/QC" pad="3"/>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D/QD" pad="4"/>
<connect gate="A" pin="E/QE" pad="9"/>
<connect gate="A" pin="F/QF" pad="10"/>
<connect gate="A" pin="G/QG" pad="11"/>
<connect gate="A" pin="G1" pad="21"/>
<connect gate="A" pin="G2" pad="20"/>
<connect gate="A" pin="H/QH" pad="12"/>
<connect gate="A" pin="QA'" pad="24"/>
<connect gate="A" pin="QH'" pad="13"/>
<connect gate="A" pin="S0" pad="23"/>
<connect gate="A" pin="S1" pad="22"/>
<connect gate="A" pin="SL" pad="17"/>
<connect gate="A" pin="SR" pad="16"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11352" prefix="IC">
<description>Dual 4 to 1 line &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411352"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="1C0" pad="16"/>
<connect gate="A" pin="1C1" pad="15"/>
<connect gate="A" pin="1C2" pad="14"/>
<connect gate="A" pin="1C3" pad="13"/>
<connect gate="A" pin="1G" pad="6"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2C0" pad="11"/>
<connect gate="A" pin="2C1" pad="10"/>
<connect gate="A" pin="2C2" pad="9"/>
<connect gate="A" pin="2C3" pad="8"/>
<connect gate="A" pin="2G" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C0" pad="16"/>
<connect gate="A" pin="1C1" pad="15"/>
<connect gate="A" pin="1C2" pad="14"/>
<connect gate="A" pin="1C3" pad="13"/>
<connect gate="A" pin="1G" pad="6"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2C0" pad="11"/>
<connect gate="A" pin="2C1" pad="10"/>
<connect gate="A" pin="2C2" pad="9"/>
<connect gate="A" pin="2C3" pad="8"/>
<connect gate="A" pin="2G" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11353" prefix="IC">
<description>Dual 4 to 1 line &lt;B&gt;DATA SELECTOR/MULTIPLEXER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411353"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="A" pin="1C0" pad="16"/>
<connect gate="A" pin="1C1" pad="15"/>
<connect gate="A" pin="1C2" pad="14"/>
<connect gate="A" pin="1C3" pad="13"/>
<connect gate="A" pin="1G" pad="6"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2C0" pad="11"/>
<connect gate="A" pin="2C1" pad="10"/>
<connect gate="A" pin="2C2" pad="9"/>
<connect gate="A" pin="2C3" pad="8"/>
<connect gate="A" pin="2G" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C0" pad="16"/>
<connect gate="A" pin="1C1" pad="15"/>
<connect gate="A" pin="1C2" pad="14"/>
<connect gate="A" pin="1C3" pad="13"/>
<connect gate="A" pin="1G" pad="6"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2C0" pad="11"/>
<connect gate="A" pin="2C1" pad="10"/>
<connect gate="A" pin="2C2" pad="9"/>
<connect gate="A" pin="2C3" pad="8"/>
<connect gate="A" pin="2G" pad="7"/>
<connect gate="A" pin="2Y" pad="5"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11373" prefix="IC">
<description>Octal transparent D-type &lt;B&gt;LATCH&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411373"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="D0" pad="23"/>
<connect gate="A" pin="D1" pad="22"/>
<connect gate="A" pin="D2" pad="21"/>
<connect gate="A" pin="D3" pad="20"/>
<connect gate="A" pin="D4" pad="17"/>
<connect gate="A" pin="D5" pad="16"/>
<connect gate="A" pin="D6" pad="15"/>
<connect gate="A" pin="D7" pad="14"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="OC" pad="24"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="D0" pad="23"/>
<connect gate="A" pin="D1" pad="22"/>
<connect gate="A" pin="D2" pad="21"/>
<connect gate="A" pin="D3" pad="20"/>
<connect gate="A" pin="D4" pad="17"/>
<connect gate="A" pin="D5" pad="16"/>
<connect gate="A" pin="D6" pad="15"/>
<connect gate="A" pin="D7" pad="14"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="OC" pad="24"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11374" prefix="IC">
<description>Octal D-type edge triggered &lt;B&gt;FLIP FLOP&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411374"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="D0" pad="23"/>
<connect gate="A" pin="D1" pad="22"/>
<connect gate="A" pin="D2" pad="21"/>
<connect gate="A" pin="D3" pad="20"/>
<connect gate="A" pin="D4" pad="17"/>
<connect gate="A" pin="D5" pad="16"/>
<connect gate="A" pin="D6" pad="15"/>
<connect gate="A" pin="D7" pad="14"/>
<connect gate="A" pin="OC" pad="24"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="D0" pad="23"/>
<connect gate="A" pin="D1" pad="22"/>
<connect gate="A" pin="D2" pad="21"/>
<connect gate="A" pin="D3" pad="20"/>
<connect gate="A" pin="D4" pad="17"/>
<connect gate="A" pin="D5" pad="16"/>
<connect gate="A" pin="D6" pad="15"/>
<connect gate="A" pin="D7" pad="14"/>
<connect gate="A" pin="OC" pad="24"/>
<connect gate="A" pin="Q0" pad="1"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11379" prefix="IC">
<description>Quadruple D-type &lt;B&gt;FLIP FLOP&lt;/B&gt;, clock enable</description>
<gates>
<gate name="A" symbol="7411379"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="!Q1" pad="1"/>
<connect gate="A" pin="!Q2" pad="3"/>
<connect gate="A" pin="!Q3" pad="8"/>
<connect gate="A" pin="!Q4" pad="10"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLKEN" pad="19"/>
<connect gate="A" pin="D1" pad="18"/>
<connect gate="A" pin="D2" pad="17"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="Q1" pad="20"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="11"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="!Q1" pad="1"/>
<connect gate="A" pin="!Q2" pad="3"/>
<connect gate="A" pin="!Q3" pad="8"/>
<connect gate="A" pin="!Q4" pad="10"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLKEN" pad="19"/>
<connect gate="A" pin="D1" pad="18"/>
<connect gate="A" pin="D2" pad="17"/>
<connect gate="A" pin="D3" pad="14"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="Q1" pad="20"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="11"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="5"/>
<connect gate="P" pin="GND@3" pad="6"/>
<connect gate="P" pin="GND@4" pad="7"/>
<connect gate="P" pin="VCC@1" pad="15"/>
<connect gate="P" pin="VCC@2" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11520" prefix="IC">
<description>8-bit &lt;B&gt;IDENTITY COMPARATOR&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411520"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="G" pad="20"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="2"/>
<connect gate="A" pin="P2" pad="19"/>
<connect gate="A" pin="P3" pad="17"/>
<connect gate="A" pin="P4" pad="14"/>
<connect gate="A" pin="P5" pad="12"/>
<connect gate="A" pin="P6" pad="10"/>
<connect gate="A" pin="P7" pad="8"/>
<connect gate="A" pin="P=Q" pad="6"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="18"/>
<connect gate="A" pin="Q3" pad="16"/>
<connect gate="A" pin="Q4" pad="13"/>
<connect gate="A" pin="Q5" pad="11"/>
<connect gate="A" pin="Q6" pad="9"/>
<connect gate="A" pin="Q7" pad="7"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="A" pin="G" pad="20"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="2"/>
<connect gate="A" pin="P2" pad="19"/>
<connect gate="A" pin="P3" pad="17"/>
<connect gate="A" pin="P4" pad="14"/>
<connect gate="A" pin="P5" pad="12"/>
<connect gate="A" pin="P6" pad="10"/>
<connect gate="A" pin="P7" pad="8"/>
<connect gate="A" pin="P=Q" pad="6"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="18"/>
<connect gate="A" pin="Q3" pad="16"/>
<connect gate="A" pin="Q4" pad="13"/>
<connect gate="A" pin="Q5" pad="11"/>
<connect gate="A" pin="Q6" pad="9"/>
<connect gate="A" pin="Q7" pad="7"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11533" prefix="IC">
<description>Octal D-type transparent &lt;B&gt;LATCH&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411533"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D1" pad="23"/>
<connect gate="A" pin="D2" pad="22"/>
<connect gate="A" pin="D3" pad="21"/>
<connect gate="A" pin="D4" pad="20"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="16"/>
<connect gate="A" pin="D7" pad="15"/>
<connect gate="A" pin="D8" pad="14"/>
<connect gate="A" pin="OE" pad="24"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="4"/>
<connect gate="A" pin="Q5" pad="9"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="11"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D1" pad="23"/>
<connect gate="A" pin="D2" pad="22"/>
<connect gate="A" pin="D3" pad="21"/>
<connect gate="A" pin="D4" pad="20"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="16"/>
<connect gate="A" pin="D7" pad="15"/>
<connect gate="A" pin="D8" pad="14"/>
<connect gate="A" pin="OE" pad="24"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="4"/>
<connect gate="A" pin="Q5" pad="9"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="11"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11534" prefix="IC">
<description>Octal D-type edge triggered &lt;B&gt;FLIP FLOP&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411534"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="D1" pad="23"/>
<connect gate="A" pin="D2" pad="22"/>
<connect gate="A" pin="D3" pad="21"/>
<connect gate="A" pin="D4" pad="20"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="16"/>
<connect gate="A" pin="D7" pad="15"/>
<connect gate="A" pin="D8" pad="14"/>
<connect gate="A" pin="OE" pad="24"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="4"/>
<connect gate="A" pin="Q5" pad="9"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="11"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="D1" pad="23"/>
<connect gate="A" pin="D2" pad="22"/>
<connect gate="A" pin="D3" pad="21"/>
<connect gate="A" pin="D4" pad="20"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="16"/>
<connect gate="A" pin="D7" pad="15"/>
<connect gate="A" pin="D8" pad="14"/>
<connect gate="A" pin="OE" pad="24"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="4"/>
<connect gate="A" pin="Q5" pad="9"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="11"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11620" prefix="IC">
<description>Octal &lt;B&gt;BUS TRANSCEIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411620"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="9"/>
<connect gate="A" pin="A6" pad="10"/>
<connect gate="A" pin="A7" pad="11"/>
<connect gate="A" pin="A8" pad="12"/>
<connect gate="A" pin="B1" pad="23"/>
<connect gate="A" pin="B2" pad="22"/>
<connect gate="A" pin="B3" pad="21"/>
<connect gate="A" pin="B4" pad="20"/>
<connect gate="A" pin="B5" pad="17"/>
<connect gate="A" pin="B6" pad="16"/>
<connect gate="A" pin="B7" pad="15"/>
<connect gate="A" pin="B8" pad="14"/>
<connect gate="A" pin="GAB" pad="24"/>
<connect gate="A" pin="GBA" pad="13"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="9"/>
<connect gate="A" pin="A6" pad="10"/>
<connect gate="A" pin="A7" pad="11"/>
<connect gate="A" pin="A8" pad="12"/>
<connect gate="A" pin="B1" pad="23"/>
<connect gate="A" pin="B2" pad="22"/>
<connect gate="A" pin="B3" pad="21"/>
<connect gate="A" pin="B4" pad="20"/>
<connect gate="A" pin="B5" pad="17"/>
<connect gate="A" pin="B6" pad="16"/>
<connect gate="A" pin="B7" pad="15"/>
<connect gate="A" pin="B8" pad="14"/>
<connect gate="A" pin="GAB" pad="24"/>
<connect gate="A" pin="GBA" pad="13"/>
<connect gate="P" pin="GND@1" pad="5"/>
<connect gate="P" pin="GND@2" pad="6"/>
<connect gate="P" pin="GND@3" pad="7"/>
<connect gate="P" pin="GND@4" pad="8"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11646" prefix="IC">
<description>Octal &lt;B&gt;BUS TRANSCEIVER/REGISTER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411646"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="10"/>
<connect gate="A" pin="A6" pad="11"/>
<connect gate="A" pin="A7" pad="12"/>
<connect gate="A" pin="A8" pad="13"/>
<connect gate="A" pin="B1" pad="26"/>
<connect gate="A" pin="B2" pad="25"/>
<connect gate="A" pin="B3" pad="24"/>
<connect gate="A" pin="B4" pad="23"/>
<connect gate="A" pin="B5" pad="20"/>
<connect gate="A" pin="B6" pad="19"/>
<connect gate="A" pin="B7" pad="18"/>
<connect gate="A" pin="B8" pad="17"/>
<connect gate="A" pin="CAB" pad="28"/>
<connect gate="A" pin="CBA" pad="16"/>
<connect gate="A" pin="DIR" pad="14"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="SAB" pad="27"/>
<connect gate="A" pin="SBA" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="10"/>
<connect gate="A" pin="A6" pad="11"/>
<connect gate="A" pin="A7" pad="12"/>
<connect gate="A" pin="A8" pad="13"/>
<connect gate="A" pin="B1" pad="26"/>
<connect gate="A" pin="B2" pad="25"/>
<connect gate="A" pin="B3" pad="24"/>
<connect gate="A" pin="B4" pad="23"/>
<connect gate="A" pin="B5" pad="20"/>
<connect gate="A" pin="B6" pad="19"/>
<connect gate="A" pin="B7" pad="18"/>
<connect gate="A" pin="B8" pad="17"/>
<connect gate="A" pin="CAB" pad="28"/>
<connect gate="A" pin="CBA" pad="16"/>
<connect gate="A" pin="DIR" pad="14"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="SAB" pad="27"/>
<connect gate="A" pin="SBA" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11651" prefix="IC">
<description>Octal &lt;B&gt;BUS TRANSCEIVER/REGISTER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411651"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="10"/>
<connect gate="A" pin="A6" pad="11"/>
<connect gate="A" pin="A7" pad="12"/>
<connect gate="A" pin="A8" pad="13"/>
<connect gate="A" pin="B1" pad="26"/>
<connect gate="A" pin="B2" pad="25"/>
<connect gate="A" pin="B3" pad="24"/>
<connect gate="A" pin="B4" pad="23"/>
<connect gate="A" pin="B5" pad="20"/>
<connect gate="A" pin="B6" pad="19"/>
<connect gate="A" pin="B7" pad="18"/>
<connect gate="A" pin="B8" pad="17"/>
<connect gate="A" pin="CAB" pad="28"/>
<connect gate="A" pin="CBA" pad="16"/>
<connect gate="A" pin="GAB" pad="1"/>
<connect gate="A" pin="GBA" pad="14"/>
<connect gate="A" pin="SAB" pad="27"/>
<connect gate="A" pin="SBA" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="10"/>
<connect gate="A" pin="A6" pad="11"/>
<connect gate="A" pin="A7" pad="12"/>
<connect gate="A" pin="A8" pad="13"/>
<connect gate="A" pin="B1" pad="26"/>
<connect gate="A" pin="B2" pad="25"/>
<connect gate="A" pin="B3" pad="24"/>
<connect gate="A" pin="B4" pad="23"/>
<connect gate="A" pin="B5" pad="20"/>
<connect gate="A" pin="B6" pad="19"/>
<connect gate="A" pin="B7" pad="18"/>
<connect gate="A" pin="B8" pad="17"/>
<connect gate="A" pin="CAB" pad="28"/>
<connect gate="A" pin="CBA" pad="16"/>
<connect gate="A" pin="GAB" pad="1"/>
<connect gate="A" pin="GBA" pad="14"/>
<connect gate="A" pin="SAB" pad="27"/>
<connect gate="A" pin="SBA" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11823" prefix="IC">
<description>9-bit bus interface &lt;B&gt;LATCH&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411823"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLKEN" pad="16"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D1" pad="27"/>
<connect gate="A" pin="D2" pad="26"/>
<connect gate="A" pin="D3" pad="25"/>
<connect gate="A" pin="D4" pad="24"/>
<connect gate="A" pin="D5" pad="23"/>
<connect gate="A" pin="D6" pad="20"/>
<connect gate="A" pin="D7" pad="19"/>
<connect gate="A" pin="D8" pad="18"/>
<connect gate="A" pin="D9" pad="17"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="4"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="11"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLKEN" pad="16"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D1" pad="27"/>
<connect gate="A" pin="D2" pad="26"/>
<connect gate="A" pin="D3" pad="25"/>
<connect gate="A" pin="D4" pad="24"/>
<connect gate="A" pin="D5" pad="23"/>
<connect gate="A" pin="D6" pad="20"/>
<connect gate="A" pin="D7" pad="19"/>
<connect gate="A" pin="D8" pad="18"/>
<connect gate="A" pin="D9" pad="17"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="4"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="11"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11824" prefix="IC">
<description>9-bit inverting bus interface &lt;B&gt;LATCH&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411824"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLKEN" pad="16"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D1" pad="27"/>
<connect gate="A" pin="D2" pad="26"/>
<connect gate="A" pin="D3" pad="25"/>
<connect gate="A" pin="D4" pad="24"/>
<connect gate="A" pin="D5" pad="23"/>
<connect gate="A" pin="D6" pad="20"/>
<connect gate="A" pin="D7" pad="19"/>
<connect gate="A" pin="D8" pad="18"/>
<connect gate="A" pin="D9" pad="17"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="4"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="11"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLKEN" pad="16"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D1" pad="27"/>
<connect gate="A" pin="D2" pad="26"/>
<connect gate="A" pin="D3" pad="25"/>
<connect gate="A" pin="D4" pad="24"/>
<connect gate="A" pin="D5" pad="23"/>
<connect gate="A" pin="D6" pad="20"/>
<connect gate="A" pin="D7" pad="19"/>
<connect gate="A" pin="D8" pad="18"/>
<connect gate="A" pin="D9" pad="17"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="A" pin="Q1" pad="1"/>
<connect gate="A" pin="Q2" pad="2"/>
<connect gate="A" pin="Q3" pad="3"/>
<connect gate="A" pin="Q4" pad="4"/>
<connect gate="A" pin="Q5" pad="5"/>
<connect gate="A" pin="Q6" pad="10"/>
<connect gate="A" pin="Q7" pad="11"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="A" pin="Q9" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11825" prefix="IC">
<description>8-bit bus interface &lt;B&gt;LATCH&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411825"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLKEN" pad="16"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D1" pad="26"/>
<connect gate="A" pin="D2" pad="25"/>
<connect gate="A" pin="D3" pad="24"/>
<connect gate="A" pin="D4" pad="23"/>
<connect gate="A" pin="D5" pad="20"/>
<connect gate="A" pin="D6" pad="19"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="D8" pad="17"/>
<connect gate="A" pin="OC1" pad="1"/>
<connect gate="A" pin="OC2" pad="28"/>
<connect gate="A" pin="OC3" pad="27"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLKEN" pad="16"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D1" pad="26"/>
<connect gate="A" pin="D2" pad="25"/>
<connect gate="A" pin="D3" pad="24"/>
<connect gate="A" pin="D4" pad="23"/>
<connect gate="A" pin="D5" pad="20"/>
<connect gate="A" pin="D6" pad="19"/>
<connect gate="A" pin="D7" pad="18"/>
<connect gate="A" pin="D8" pad="17"/>
<connect gate="A" pin="OC1" pad="1"/>
<connect gate="A" pin="OC2" pad="28"/>
<connect gate="A" pin="OC3" pad="27"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11827" prefix="IC">
<description>10-bit &lt;B&gt;BUFFER/BUS DRIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411827"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="A1" pad="27"/>
<connect gate="A" pin="A10" pad="16"/>
<connect gate="A" pin="A2" pad="26"/>
<connect gate="A" pin="A3" pad="25"/>
<connect gate="A" pin="A4" pad="24"/>
<connect gate="A" pin="A5" pad="23"/>
<connect gate="A" pin="A6" pad="20"/>
<connect gate="A" pin="A7" pad="19"/>
<connect gate="A" pin="A8" pad="18"/>
<connect gate="A" pin="A9" pad="17"/>
<connect gate="A" pin="G1" pad="28"/>
<connect gate="A" pin="G2" pad="15"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y10" pad="14"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="4"/>
<connect gate="A" pin="Y5" pad="5"/>
<connect gate="A" pin="Y6" pad="10"/>
<connect gate="A" pin="Y7" pad="11"/>
<connect gate="A" pin="Y8" pad="12"/>
<connect gate="A" pin="Y9" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="A1" pad="27"/>
<connect gate="A" pin="A10" pad="16"/>
<connect gate="A" pin="A2" pad="26"/>
<connect gate="A" pin="A3" pad="25"/>
<connect gate="A" pin="A4" pad="24"/>
<connect gate="A" pin="A5" pad="23"/>
<connect gate="A" pin="A6" pad="20"/>
<connect gate="A" pin="A7" pad="19"/>
<connect gate="A" pin="A8" pad="18"/>
<connect gate="A" pin="A9" pad="17"/>
<connect gate="A" pin="G1" pad="28"/>
<connect gate="A" pin="G2" pad="15"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y10" pad="14"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="4"/>
<connect gate="A" pin="Y5" pad="5"/>
<connect gate="A" pin="Y6" pad="10"/>
<connect gate="A" pin="Y7" pad="11"/>
<connect gate="A" pin="Y8" pad="12"/>
<connect gate="A" pin="Y9" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11833" prefix="IC">
<description>&lt;B&gt;PARITY GENERATOR/CHECKER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411833"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="10"/>
<connect gate="A" pin="A6" pad="11"/>
<connect gate="A" pin="A7" pad="12"/>
<connect gate="A" pin="A8" pad="13"/>
<connect gate="A" pin="B1" pad="26"/>
<connect gate="A" pin="B2" pad="25"/>
<connect gate="A" pin="B3" pad="24"/>
<connect gate="A" pin="B4" pad="23"/>
<connect gate="A" pin="B5" pad="20"/>
<connect gate="A" pin="B6" pad="19"/>
<connect gate="A" pin="B7" pad="18"/>
<connect gate="A" pin="B8" pad="17"/>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLR" pad="16"/>
<connect gate="A" pin="ERR" pad="14"/>
<connect gate="A" pin="OEA" pad="28"/>
<connect gate="A" pin="OEB" pad="27"/>
<connect gate="A" pin="PAR" pad="1"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="10"/>
<connect gate="A" pin="A6" pad="11"/>
<connect gate="A" pin="A7" pad="12"/>
<connect gate="A" pin="A8" pad="13"/>
<connect gate="A" pin="B1" pad="26"/>
<connect gate="A" pin="B2" pad="25"/>
<connect gate="A" pin="B3" pad="24"/>
<connect gate="A" pin="B4" pad="23"/>
<connect gate="A" pin="B5" pad="20"/>
<connect gate="A" pin="B6" pad="19"/>
<connect gate="A" pin="B7" pad="18"/>
<connect gate="A" pin="B8" pad="17"/>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLR" pad="16"/>
<connect gate="A" pin="ERR" pad="14"/>
<connect gate="A" pin="OEA" pad="28"/>
<connect gate="A" pin="OEB" pad="27"/>
<connect gate="A" pin="PAR" pad="1"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11861" prefix="IC">
<description>10-bit &lt;B&gt;BUS BUFFER&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411861"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A10" pad="14"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="10"/>
<connect gate="A" pin="A7" pad="11"/>
<connect gate="A" pin="A8" pad="12"/>
<connect gate="A" pin="A9" pad="13"/>
<connect gate="A" pin="B1" pad="27"/>
<connect gate="A" pin="B10" pad="16"/>
<connect gate="A" pin="B2" pad="26"/>
<connect gate="A" pin="B3" pad="25"/>
<connect gate="A" pin="B4" pad="24"/>
<connect gate="A" pin="B5" pad="23"/>
<connect gate="A" pin="B6" pad="20"/>
<connect gate="A" pin="B7" pad="19"/>
<connect gate="A" pin="B8" pad="18"/>
<connect gate="A" pin="B9" pad="17"/>
<connect gate="A" pin="GAB" pad="15"/>
<connect gate="A" pin="GBA" pad="28"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A10" pad="14"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="10"/>
<connect gate="A" pin="A7" pad="11"/>
<connect gate="A" pin="A8" pad="12"/>
<connect gate="A" pin="A9" pad="13"/>
<connect gate="A" pin="B1" pad="27"/>
<connect gate="A" pin="B10" pad="16"/>
<connect gate="A" pin="B2" pad="26"/>
<connect gate="A" pin="B3" pad="25"/>
<connect gate="A" pin="B4" pad="24"/>
<connect gate="A" pin="B5" pad="23"/>
<connect gate="A" pin="B6" pad="20"/>
<connect gate="A" pin="B7" pad="19"/>
<connect gate="A" pin="B8" pad="18"/>
<connect gate="A" pin="B9" pad="17"/>
<connect gate="A" pin="GAB" pad="15"/>
<connect gate="A" pin="GBA" pad="28"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11882" prefix="IC">
<description>&lt;B&gt;COMPARATOR&lt;/B&gt;</description>
<gates>
<gate name="A" symbol="7411882"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="A" pin="CN" pad="3"/>
<connect gate="A" pin="CN+16" pad="5"/>
<connect gate="A" pin="CN+24" pad="10"/>
<connect gate="A" pin="CN+32" pad="11"/>
<connect gate="A" pin="CN+8" pad="4"/>
<connect gate="A" pin="G0" pad="1"/>
<connect gate="A" pin="G1" pad="27"/>
<connect gate="A" pin="G2" pad="25"/>
<connect gate="A" pin="G3" pad="23"/>
<connect gate="A" pin="G4" pad="19"/>
<connect gate="A" pin="G5" pad="17"/>
<connect gate="A" pin="G6" pad="15"/>
<connect gate="A" pin="G7" pad="13"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="28"/>
<connect gate="A" pin="P2" pad="26"/>
<connect gate="A" pin="P3" pad="24"/>
<connect gate="A" pin="P4" pad="20"/>
<connect gate="A" pin="P5" pad="18"/>
<connect gate="A" pin="P6" pad="16"/>
<connect gate="A" pin="P7" pad="14"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="CN" pad="3"/>
<connect gate="A" pin="CN+16" pad="5"/>
<connect gate="A" pin="CN+24" pad="10"/>
<connect gate="A" pin="CN+32" pad="11"/>
<connect gate="A" pin="CN+8" pad="4"/>
<connect gate="A" pin="G0" pad="1"/>
<connect gate="A" pin="G1" pad="27"/>
<connect gate="A" pin="G2" pad="25"/>
<connect gate="A" pin="G3" pad="23"/>
<connect gate="A" pin="G4" pad="19"/>
<connect gate="A" pin="G5" pad="17"/>
<connect gate="A" pin="G6" pad="15"/>
<connect gate="A" pin="G7" pad="13"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="28"/>
<connect gate="A" pin="P2" pad="26"/>
<connect gate="A" pin="P3" pad="24"/>
<connect gate="A" pin="P4" pad="20"/>
<connect gate="A" pin="P5" pad="18"/>
<connect gate="A" pin="P6" pad="16"/>
<connect gate="A" pin="P7" pad="14"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11853" prefix="IC">
<description>&lt;B&gt;PARITY GENERATOR/CHECKER&lt;/B&gt;</description>
<gates>
<gate name="P1" symbol="7411853"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
<connect gate="P1" pin="A1" pad="2"/>
<connect gate="P1" pin="A2" pad="3"/>
<connect gate="P1" pin="A3" pad="4"/>
<connect gate="P1" pin="A4" pad="5"/>
<connect gate="P1" pin="A5" pad="10"/>
<connect gate="P1" pin="A6" pad="11"/>
<connect gate="P1" pin="A7" pad="12"/>
<connect gate="P1" pin="A8" pad="13"/>
<connect gate="P1" pin="B1" pad="26"/>
<connect gate="P1" pin="B2" pad="25"/>
<connect gate="P1" pin="B3" pad="24"/>
<connect gate="P1" pin="B4" pad="23"/>
<connect gate="P1" pin="B5" pad="20"/>
<connect gate="P1" pin="B6" pad="19"/>
<connect gate="P1" pin="B7" pad="18"/>
<connect gate="P1" pin="B8" pad="17"/>
<connect gate="P1" pin="CLR" pad="16"/>
<connect gate="P1" pin="ERR" pad="14"/>
<connect gate="P1" pin="LE" pad="15"/>
<connect gate="P1" pin="OEA" pad="28"/>
<connect gate="P1" pin="OEB" pad="27"/>
<connect gate="P1" pin="PAR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
<connect gate="P1" pin="A1" pad="2"/>
<connect gate="P1" pin="A2" pad="3"/>
<connect gate="P1" pin="A3" pad="4"/>
<connect gate="P1" pin="A4" pad="5"/>
<connect gate="P1" pin="A5" pad="10"/>
<connect gate="P1" pin="A6" pad="11"/>
<connect gate="P1" pin="A7" pad="12"/>
<connect gate="P1" pin="A8" pad="13"/>
<connect gate="P1" pin="B1" pad="26"/>
<connect gate="P1" pin="B2" pad="25"/>
<connect gate="P1" pin="B3" pad="24"/>
<connect gate="P1" pin="B4" pad="23"/>
<connect gate="P1" pin="B5" pad="20"/>
<connect gate="P1" pin="B6" pad="19"/>
<connect gate="P1" pin="B7" pad="18"/>
<connect gate="P1" pin="B8" pad="17"/>
<connect gate="P1" pin="CLR" pad="16"/>
<connect gate="P1" pin="ERR" pad="14"/>
<connect gate="P1" pin="LE" pad="15"/>
<connect gate="P1" pin="OEA" pad="28"/>
<connect gate="P1" pin="OEB" pad="27"/>
<connect gate="P1" pin="PAR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11648" prefix="IC">
<description>Octal &lt;B&gt;BUS TRANSCEIVER/REGISTER&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="7411648"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="10"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="12"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="B1" pad="26"/>
<connect gate="G$1" pin="B2" pad="25"/>
<connect gate="G$1" pin="B3" pad="24"/>
<connect gate="G$1" pin="B4" pad="23"/>
<connect gate="G$1" pin="B5" pad="20"/>
<connect gate="G$1" pin="B6" pad="19"/>
<connect gate="G$1" pin="B7" pad="18"/>
<connect gate="G$1" pin="B8" pad="17"/>
<connect gate="G$1" pin="CAB" pad="28"/>
<connect gate="G$1" pin="CBA" pad="16"/>
<connect gate="G$1" pin="DIR" pad="14"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="SAB" pad="27"/>
<connect gate="G$1" pin="SBA" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="10"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="12"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="B1" pad="26"/>
<connect gate="G$1" pin="B2" pad="25"/>
<connect gate="G$1" pin="B3" pad="24"/>
<connect gate="G$1" pin="B4" pad="23"/>
<connect gate="G$1" pin="B5" pad="20"/>
<connect gate="G$1" pin="B6" pad="19"/>
<connect gate="G$1" pin="B7" pad="18"/>
<connect gate="G$1" pin="B8" pad="17"/>
<connect gate="G$1" pin="CAB" pad="28"/>
<connect gate="G$1" pin="CBA" pad="16"/>
<connect gate="G$1" pin="DIR" pad="14"/>
<connect gate="G$1" pin="G" pad="1"/>
<connect gate="G$1" pin="SAB" pad="27"/>
<connect gate="G$1" pin="SBA" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11652" prefix="IC">
<description>Octal &lt;B&gt;BUS TRANSCEIVER/REGISTER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7411652"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="10"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="12"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="B1" pad="26"/>
<connect gate="G$1" pin="B2" pad="25"/>
<connect gate="G$1" pin="B3" pad="24"/>
<connect gate="G$1" pin="B4" pad="23"/>
<connect gate="G$1" pin="B5" pad="20"/>
<connect gate="G$1" pin="B6" pad="19"/>
<connect gate="G$1" pin="B7" pad="18"/>
<connect gate="G$1" pin="B8" pad="17"/>
<connect gate="G$1" pin="CAB" pad="28"/>
<connect gate="G$1" pin="CBA" pad="16"/>
<connect gate="G$1" pin="G-BA" pad="14"/>
<connect gate="G$1" pin="GAB" pad="1"/>
<connect gate="G$1" pin="SAB" pad="27"/>
<connect gate="G$1" pin="SBA" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="10"/>
<connect gate="G$1" pin="A6" pad="11"/>
<connect gate="G$1" pin="A7" pad="12"/>
<connect gate="G$1" pin="A8" pad="13"/>
<connect gate="G$1" pin="B1" pad="26"/>
<connect gate="G$1" pin="B2" pad="25"/>
<connect gate="G$1" pin="B3" pad="24"/>
<connect gate="G$1" pin="B4" pad="23"/>
<connect gate="G$1" pin="B5" pad="20"/>
<connect gate="G$1" pin="B6" pad="19"/>
<connect gate="G$1" pin="B7" pad="18"/>
<connect gate="G$1" pin="B8" pad="17"/>
<connect gate="G$1" pin="CAB" pad="28"/>
<connect gate="G$1" pin="CBA" pad="16"/>
<connect gate="G$1" pin="G-BA" pad="14"/>
<connect gate="G$1" pin="GAB" pad="1"/>
<connect gate="G$1" pin="SAB" pad="27"/>
<connect gate="G$1" pin="SBA" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11873" prefix="IC">
<description>Dual 4-bit D type &lt;B&gt;LATCH&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411873"/>
<gate name="B" symbol="7411873"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="CLR" pad="27"/>
<connect gate="A" pin="D1" pad="26"/>
<connect gate="A" pin="D2" pad="25"/>
<connect gate="A" pin="D3" pad="24"/>
<connect gate="A" pin="D4" pad="23"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="B" pin="C" pad="14"/>
<connect gate="B" pin="CLR" pad="16"/>
<connect gate="B" pin="D1" pad="20"/>
<connect gate="B" pin="D2" pad="19"/>
<connect gate="B" pin="D3" pad="18"/>
<connect gate="B" pin="D4" pad="17"/>
<connect gate="B" pin="OC" pad="15"/>
<connect gate="B" pin="Q1" pad="10"/>
<connect gate="B" pin="Q2" pad="11"/>
<connect gate="B" pin="Q3" pad="12"/>
<connect gate="B" pin="Q4" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="CLR" pad="27"/>
<connect gate="A" pin="D1" pad="26"/>
<connect gate="A" pin="D2" pad="25"/>
<connect gate="A" pin="D3" pad="24"/>
<connect gate="A" pin="D4" pad="23"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="B" pin="C" pad="14"/>
<connect gate="B" pin="CLR" pad="16"/>
<connect gate="B" pin="D1" pad="20"/>
<connect gate="B" pin="D2" pad="19"/>
<connect gate="B" pin="D3" pad="18"/>
<connect gate="B" pin="D4" pad="17"/>
<connect gate="B" pin="OC" pad="15"/>
<connect gate="B" pin="Q1" pad="10"/>
<connect gate="B" pin="Q2" pad="11"/>
<connect gate="B" pin="Q3" pad="12"/>
<connect gate="B" pin="Q4" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11874" prefix="IC">
<description>Dual 4-bit D type edge triggered &lt;B&gt;FLIP FLOP&lt;/B&gt;, 3-state</description>
<gates>
<gate name="A" symbol="7411874"/>
<gate name="B" symbol="7411874"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="27"/>
<connect gate="A" pin="D1" pad="26"/>
<connect gate="A" pin="D2" pad="25"/>
<connect gate="A" pin="D3" pad="24"/>
<connect gate="A" pin="D4" pad="23"/>
<connect gate="A" pin="OE" pad="28"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="B" pin="CLK" pad="14"/>
<connect gate="B" pin="CLR" pad="16"/>
<connect gate="B" pin="D1" pad="20"/>
<connect gate="B" pin="D2" pad="19"/>
<connect gate="B" pin="D3" pad="18"/>
<connect gate="B" pin="D4" pad="17"/>
<connect gate="B" pin="OE" pad="15"/>
<connect gate="B" pin="Q1" pad="10"/>
<connect gate="B" pin="Q2" pad="11"/>
<connect gate="B" pin="Q3" pad="12"/>
<connect gate="B" pin="Q4" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="27"/>
<connect gate="A" pin="D1" pad="26"/>
<connect gate="A" pin="D2" pad="25"/>
<connect gate="A" pin="D3" pad="24"/>
<connect gate="A" pin="D4" pad="23"/>
<connect gate="A" pin="OE" pad="28"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="4"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="B" pin="CLK" pad="14"/>
<connect gate="B" pin="CLR" pad="16"/>
<connect gate="B" pin="D1" pad="20"/>
<connect gate="B" pin="D2" pad="19"/>
<connect gate="B" pin="D3" pad="18"/>
<connect gate="B" pin="D4" pad="17"/>
<connect gate="B" pin="OE" pad="15"/>
<connect gate="B" pin="Q1" pad="10"/>
<connect gate="B" pin="Q2" pad="11"/>
<connect gate="B" pin="Q3" pad="12"/>
<connect gate="B" pin="Q4" pad="13"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC11881" prefix="IC">
<description>&lt;B&gt;COMPARATOR&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="7411881"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="A0" pad="28"/>
<connect gate="G$1" pin="A1" pad="27"/>
<connect gate="G$1" pin="A2" pad="26"/>
<connect gate="G$1" pin="A3" pad="25"/>
<connect gate="G$1" pin="A=B" pad="3"/>
<connect gate="G$1" pin="B0" pad="24"/>
<connect gate="G$1" pin="B1" pad="23"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="19"/>
<connect gate="G$1" pin="CN" pad="1"/>
<connect gate="G$1" pin="CN+4" pad="14"/>
<connect gate="G$1" pin="F0" pad="4"/>
<connect gate="G$1" pin="F1" pad="5"/>
<connect gate="G$1" pin="F2" pad="10"/>
<connect gate="G$1" pin="F3" pad="11"/>
<connect gate="G$1" pin="G" pad="13"/>
<connect gate="G$1" pin="M" pad="2"/>
<connect gate="G$1" pin="P" pad="12"/>
<connect gate="G$1" pin="S0" pad="18"/>
<connect gate="G$1" pin="S1" pad="17"/>
<connect gate="G$1" pin="S2" pad="16"/>
<connect gate="G$1" pin="S3" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="G$1" pin="A0" pad="28"/>
<connect gate="G$1" pin="A1" pad="27"/>
<connect gate="G$1" pin="A2" pad="26"/>
<connect gate="G$1" pin="A3" pad="25"/>
<connect gate="G$1" pin="A=B" pad="3"/>
<connect gate="G$1" pin="B0" pad="24"/>
<connect gate="G$1" pin="B1" pad="23"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="19"/>
<connect gate="G$1" pin="CN" pad="1"/>
<connect gate="G$1" pin="CN+4" pad="14"/>
<connect gate="G$1" pin="F0" pad="4"/>
<connect gate="G$1" pin="F1" pad="5"/>
<connect gate="G$1" pin="F2" pad="10"/>
<connect gate="G$1" pin="F3" pad="11"/>
<connect gate="G$1" pin="G" pad="13"/>
<connect gate="G$1" pin="M" pad="2"/>
<connect gate="G$1" pin="P" pad="12"/>
<connect gate="G$1" pin="S0" pad="18"/>
<connect gate="G$1" pin="S1" pad="17"/>
<connect gate="G$1" pin="S2" pad="16"/>
<connect gate="G$1" pin="S3" pad="15"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC16240" prefix="IC">
<description>16-bit &lt;B&gt;BUS DRIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7416240"/>
<gate name="P" symbol="4PWR8GND"/>
</gates>
<devices>
<device name="" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1G" pad="1"/>
<connect gate="G$1" pin="1Y1" pad="2"/>
<connect gate="G$1" pin="1Y2" pad="3"/>
<connect gate="G$1" pin="1Y3" pad="5"/>
<connect gate="G$1" pin="1Y4" pad="6"/>
<connect gate="G$1" pin="2A1" pad="41"/>
<connect gate="G$1" pin="2A2" pad="40"/>
<connect gate="G$1" pin="2A3" pad="38"/>
<connect gate="G$1" pin="2A4" pad="37"/>
<connect gate="G$1" pin="2G" pad="48"/>
<connect gate="G$1" pin="2Y1" pad="8"/>
<connect gate="G$1" pin="2Y2" pad="9"/>
<connect gate="G$1" pin="2Y3" pad="11"/>
<connect gate="G$1" pin="2Y4" pad="12"/>
<connect gate="G$1" pin="3A1" pad="36"/>
<connect gate="G$1" pin="3A2" pad="35"/>
<connect gate="G$1" pin="3A3" pad="33"/>
<connect gate="G$1" pin="3A4" pad="32"/>
<connect gate="G$1" pin="3G" pad="25"/>
<connect gate="G$1" pin="3Y1" pad="13"/>
<connect gate="G$1" pin="3Y2" pad="14"/>
<connect gate="G$1" pin="3Y3" pad="16"/>
<connect gate="G$1" pin="3Y4" pad="17"/>
<connect gate="G$1" pin="4A1" pad="30"/>
<connect gate="G$1" pin="4A2" pad="29"/>
<connect gate="G$1" pin="4A3" pad="27"/>
<connect gate="G$1" pin="4A4" pad="26"/>
<connect gate="G$1" pin="4G" pad="24"/>
<connect gate="G$1" pin="4Y1" pad="19"/>
<connect gate="G$1" pin="4Y2" pad="20"/>
<connect gate="G$1" pin="4Y3" pad="22"/>
<connect gate="G$1" pin="4Y4" pad="23"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC16244" prefix="IC">
<description>16-bit &lt;B&gt;BUFFER/LINE DRIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7416244"/>
<gate name="P" symbol="4PWR8GND"/>
</gates>
<devices>
<device name="" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1G" pad="1"/>
<connect gate="G$1" pin="1Y1" pad="2"/>
<connect gate="G$1" pin="1Y2" pad="3"/>
<connect gate="G$1" pin="1Y3" pad="5"/>
<connect gate="G$1" pin="1Y4" pad="6"/>
<connect gate="G$1" pin="2A1" pad="41"/>
<connect gate="G$1" pin="2A2" pad="40"/>
<connect gate="G$1" pin="2A3" pad="38"/>
<connect gate="G$1" pin="2A4" pad="37"/>
<connect gate="G$1" pin="2G" pad="48"/>
<connect gate="G$1" pin="2Y1" pad="8"/>
<connect gate="G$1" pin="2Y2" pad="9"/>
<connect gate="G$1" pin="2Y3" pad="11"/>
<connect gate="G$1" pin="2Y4" pad="12"/>
<connect gate="G$1" pin="3A1" pad="36"/>
<connect gate="G$1" pin="3A2" pad="35"/>
<connect gate="G$1" pin="3A3" pad="33"/>
<connect gate="G$1" pin="3A4" pad="32"/>
<connect gate="G$1" pin="3G" pad="25"/>
<connect gate="G$1" pin="3Y1" pad="13"/>
<connect gate="G$1" pin="3Y2" pad="14"/>
<connect gate="G$1" pin="3Y3" pad="16"/>
<connect gate="G$1" pin="3Y4" pad="17"/>
<connect gate="G$1" pin="4A1" pad="30"/>
<connect gate="G$1" pin="4A2" pad="29"/>
<connect gate="G$1" pin="4A3" pad="27"/>
<connect gate="G$1" pin="4A4" pad="26"/>
<connect gate="G$1" pin="4G" pad="24"/>
<connect gate="G$1" pin="4Y1" pad="19"/>
<connect gate="G$1" pin="4Y2" pad="20"/>
<connect gate="G$1" pin="4Y3" pad="22"/>
<connect gate="G$1" pin="4Y4" pad="23"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC16245" prefix="IC">
<description>16-bit &lt;B&gt;BUS TRANSCEIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7416245"/>
<gate name="P" symbol="4PWR8GND"/>
</gates>
<devices>
<device name="" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1A5" pad="41"/>
<connect gate="G$1" pin="1A6" pad="40"/>
<connect gate="G$1" pin="1A7" pad="38"/>
<connect gate="G$1" pin="1A8" pad="37"/>
<connect gate="G$1" pin="1B1" pad="2"/>
<connect gate="G$1" pin="1B2" pad="3"/>
<connect gate="G$1" pin="1B3" pad="5"/>
<connect gate="G$1" pin="1B4" pad="6"/>
<connect gate="G$1" pin="1B5" pad="8"/>
<connect gate="G$1" pin="1B6" pad="9"/>
<connect gate="G$1" pin="1B7" pad="11"/>
<connect gate="G$1" pin="1B8" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="1"/>
<connect gate="G$1" pin="1G" pad="48"/>
<connect gate="G$1" pin="2A1" pad="36"/>
<connect gate="G$1" pin="2A2" pad="35"/>
<connect gate="G$1" pin="2A3" pad="33"/>
<connect gate="G$1" pin="2A4" pad="32"/>
<connect gate="G$1" pin="2A5" pad="30"/>
<connect gate="G$1" pin="2A6" pad="29"/>
<connect gate="G$1" pin="2A7" pad="27"/>
<connect gate="G$1" pin="2A8" pad="26"/>
<connect gate="G$1" pin="2B1" pad="13"/>
<connect gate="G$1" pin="2B2" pad="14"/>
<connect gate="G$1" pin="2B3" pad="16"/>
<connect gate="G$1" pin="2B4" pad="17"/>
<connect gate="G$1" pin="2B5" pad="19"/>
<connect gate="G$1" pin="2B6" pad="20"/>
<connect gate="G$1" pin="2B7" pad="22"/>
<connect gate="G$1" pin="2B8" pad="23"/>
<connect gate="G$1" pin="2DIR" pad="24"/>
<connect gate="G$1" pin="2G" pad="25"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC16373" prefix="IC">
<description>16-bit transparent D-type &lt;B&gt;LATCH&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7416373"/>
<gate name="P" symbol="4PWR8GND"/>
</gates>
<devices>
<device name="" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="1C" pad="48"/>
<connect gate="G$1" pin="1D1" pad="47"/>
<connect gate="G$1" pin="1D2" pad="46"/>
<connect gate="G$1" pin="1D3" pad="44"/>
<connect gate="G$1" pin="1D4" pad="43"/>
<connect gate="G$1" pin="1D5" pad="41"/>
<connect gate="G$1" pin="1D6" pad="40"/>
<connect gate="G$1" pin="1D7" pad="38"/>
<connect gate="G$1" pin="1D8" pad="37"/>
<connect gate="G$1" pin="1OE" pad="1"/>
<connect gate="G$1" pin="1Q1" pad="2"/>
<connect gate="G$1" pin="1Q2" pad="3"/>
<connect gate="G$1" pin="1Q3" pad="5"/>
<connect gate="G$1" pin="1Q4" pad="6"/>
<connect gate="G$1" pin="1Q5" pad="8"/>
<connect gate="G$1" pin="1Q6" pad="9"/>
<connect gate="G$1" pin="1Q7" pad="11"/>
<connect gate="G$1" pin="1Q8" pad="12"/>
<connect gate="G$1" pin="2C" pad="25"/>
<connect gate="G$1" pin="2D1" pad="36"/>
<connect gate="G$1" pin="2D2" pad="35"/>
<connect gate="G$1" pin="2D3" pad="33"/>
<connect gate="G$1" pin="2D4" pad="32"/>
<connect gate="G$1" pin="2D5" pad="30"/>
<connect gate="G$1" pin="2D6" pad="29"/>
<connect gate="G$1" pin="2D7" pad="27"/>
<connect gate="G$1" pin="2D8" pad="26"/>
<connect gate="G$1" pin="2OE" pad="24"/>
<connect gate="G$1" pin="2Q1" pad="13"/>
<connect gate="G$1" pin="2Q2" pad="14"/>
<connect gate="G$1" pin="2Q3" pad="16"/>
<connect gate="G$1" pin="2Q4" pad="17"/>
<connect gate="G$1" pin="2Q5" pad="19"/>
<connect gate="G$1" pin="2Q6" pad="20"/>
<connect gate="G$1" pin="2Q7" pad="22"/>
<connect gate="G$1" pin="2Q8" pad="23"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC16374" prefix="IC">
<description>16-bit edge-triggered D-type &lt;B&gt;FLIP FLOP&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7416374"/>
<gate name="P" symbol="4PWR8GND"/>
</gates>
<devices>
<device name="" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="1CLK" pad="48"/>
<connect gate="G$1" pin="1D1" pad="47"/>
<connect gate="G$1" pin="1D2" pad="46"/>
<connect gate="G$1" pin="1D3" pad="44"/>
<connect gate="G$1" pin="1D4" pad="43"/>
<connect gate="G$1" pin="1D5" pad="41"/>
<connect gate="G$1" pin="1D6" pad="40"/>
<connect gate="G$1" pin="1D7" pad="38"/>
<connect gate="G$1" pin="1D8" pad="37"/>
<connect gate="G$1" pin="1OE" pad="1"/>
<connect gate="G$1" pin="1Q1" pad="2"/>
<connect gate="G$1" pin="1Q2" pad="3"/>
<connect gate="G$1" pin="1Q3" pad="5"/>
<connect gate="G$1" pin="1Q4" pad="6"/>
<connect gate="G$1" pin="1Q5" pad="8"/>
<connect gate="G$1" pin="1Q6" pad="9"/>
<connect gate="G$1" pin="1Q7" pad="11"/>
<connect gate="G$1" pin="1Q8" pad="12"/>
<connect gate="G$1" pin="2CLK" pad="25"/>
<connect gate="G$1" pin="2D1" pad="36"/>
<connect gate="G$1" pin="2D2" pad="35"/>
<connect gate="G$1" pin="2D3" pad="33"/>
<connect gate="G$1" pin="2D4" pad="32"/>
<connect gate="G$1" pin="2D5" pad="30"/>
<connect gate="G$1" pin="2D6" pad="29"/>
<connect gate="G$1" pin="2D7" pad="27"/>
<connect gate="G$1" pin="2D8" pad="26"/>
<connect gate="G$1" pin="2OE" pad="24"/>
<connect gate="G$1" pin="2Q1" pad="13"/>
<connect gate="G$1" pin="2Q2" pad="14"/>
<connect gate="G$1" pin="2Q3" pad="16"/>
<connect gate="G$1" pin="2Q4" pad="17"/>
<connect gate="G$1" pin="2Q5" pad="19"/>
<connect gate="G$1" pin="2Q6" pad="20"/>
<connect gate="G$1" pin="2Q7" pad="22"/>
<connect gate="G$1" pin="2Q8" pad="23"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74AC16620" prefix="IC">
<description>16-bit &lt;B&gt;BUS TRANSCEIVER&lt;/B&gt;, 3-state</description>
<gates>
<gate name="G$1" symbol="7416620"/>
<gate name="P" symbol="4PWR8GND"/>
</gates>
<devices>
<device name="" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1A5" pad="41"/>
<connect gate="G$1" pin="1A6" pad="40"/>
<connect gate="G$1" pin="1A7" pad="38"/>
<connect gate="G$1" pin="1A8" pad="37"/>
<connect gate="G$1" pin="1B1" pad="2"/>
<connect gate="G$1" pin="1B2" pad="3"/>
<connect gate="G$1" pin="1B3" pad="5"/>
<connect gate="G$1" pin="1B4" pad="6"/>
<connect gate="G$1" pin="1B5" pad="8"/>
<connect gate="G$1" pin="1B6" pad="9"/>
<connect gate="G$1" pin="1B7" pad="11"/>
<connect gate="G$1" pin="1B8" pad="12"/>
<connect gate="G$1" pin="1GAB" pad="1"/>
<connect gate="G$1" pin="1GBA" pad="48"/>
<connect gate="G$1" pin="2A1" pad="36"/>
<connect gate="G$1" pin="2A2" pad="35"/>
<connect gate="G$1" pin="2A3" pad="33"/>
<connect gate="G$1" pin="2A4" pad="32"/>
<connect gate="G$1" pin="2A5" pad="30"/>
<connect gate="G$1" pin="2A6" pad="29"/>
<connect gate="G$1" pin="2A7" pad="27"/>
<connect gate="G$1" pin="2A8" pad="26"/>
<connect gate="G$1" pin="2B1" pad="13"/>
<connect gate="G$1" pin="2B2" pad="14"/>
<connect gate="G$1" pin="2B3" pad="16"/>
<connect gate="G$1" pin="2B4" pad="17"/>
<connect gate="G$1" pin="2B5" pad="19"/>
<connect gate="G$1" pin="2B6" pad="20"/>
<connect gate="G$1" pin="2B7" pad="22"/>
<connect gate="G$1" pin="2B8" pad="23"/>
<connect gate="G$1" pin="2GAB" pad="24"/>
<connect gate="G$1" pin="2GBA" pad="25"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="GND@2" pad="10"/>
<connect gate="P" pin="GND@3" pad="15"/>
<connect gate="P" pin="GND@4" pad="21"/>
<connect gate="P" pin="GND@5" pad="28"/>
<connect gate="P" pin="GND@6" pad="34"/>
<connect gate="P" pin="GND@7" pad="39"/>
<connect gate="P" pin="GND@8" pad="45"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="31"/>
<connect gate="P" pin="VCC@4" pad="42"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
