<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<library>
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
<package name="SO24W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="PLCC68">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;</description>
</package>
<package name="PLCC20">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;&lt;p&gt;IPC standard</description>
</package>
<package name="PLCC28">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;&lt;p&gt;IPC standard</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="LCC28">
<description>&lt;b&gt;Leadless Chip Carrier&lt;/b&gt;&lt;p&gt; Ceramic Package</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL48">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO16D">
<description>&lt;b&gt;Platic Small Outline&lt;/b&gt; D R-PDSO-G16&lt;p&gt;
Source: www.ti.com .. cd74hct191.pdf</description>
</package>
<package name="SO-16LD">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; 300 x 400 mil</description>
</package>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
<package name="SO14PW">
<description>&lt;b&gt;SO14-pw&lt;/b&gt; R-PDSO-G&lt;p&gt;
Source: cd74hct191.pdf</description>
</package>
<package name="SO16PW">
<description>&lt;b&gt;SO16-pw&lt;/b&gt; R-PDSO-G&lt;p&gt;
Source: www.ti.com .. cd74hct191.pdf</description>
</package>
<package name="SO16NS">
<description>&lt;b&gt;Platic Small Outline&lt;/b&gt; NS R-PDSO-G16&lt;p&gt;
Source: www.ti.com .. cd74hct191.pdf</description>
</package>
<package name="SO20W">
<description>&lt;b&gt;Wide Small Outline package&lt;/b&gt; 300 mil</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;plastic thin shrink small outline package; 14 leads; body width 4.4 mm&lt;/b&gt;&lt;p&gt;
SOT402-1&lt;br&gt;
Source: http://www.nxp.com/documents/data_sheet/74ABT125.pdf</description>
</package>
<package name="SSOP14">
<description>&lt;b&gt;plastic shrink small outline package; 14 leads; body width 5.3 mm&lt;/b&gt;&lt;p&gt;
SOT337-1&lt;br&gt;
Source: http://www.nxp.com/documents/data_sheet/74ABT125.pdf</description>
</package>
<package name="DHVQFN14">
<description>&lt;b&gt;plastic dual in-line compatible thermal enhanced very thin quad flat package; no leads; 14 terminals; body 2.5 x 3 x 0.85 mm&lt;/b&gt;&lt;p&gt;
Source: http://www.nxp.com/documents/data_sheet/74ABT125.pdf</description>
</package>
</packages>
<symbols>
<symbol name="7404">
<pin name="I" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7405">
<pin name="I" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="7407">
<pin name="I" direction="in"/>
<pin name="O" direction="oc"/>
</symbol>
<symbol name="7442">
<pin name="O0" direction="out" function="dot"/>
<pin name="O1" direction="out" function="dot"/>
<pin name="O2" direction="out" function="dot"/>
<pin name="O3" direction="out" function="dot"/>
<pin name="O4" direction="out" function="dot"/>
<pin name="O5" direction="out" function="dot"/>
<pin name="O6" direction="out" function="dot"/>
<pin name="O7" direction="out" function="dot"/>
<pin name="O8" direction="out" function="dot"/>
<pin name="O9" direction="out" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="7445">
<pin name="O0" direction="oc" function="dot"/>
<pin name="O1" direction="oc" function="dot"/>
<pin name="O2" direction="oc" function="dot"/>
<pin name="O3" direction="oc" function="dot"/>
<pin name="O4" direction="oc" function="dot"/>
<pin name="O5" direction="oc" function="dot"/>
<pin name="O6" direction="oc" function="dot"/>
<pin name="O7" direction="oc" function="dot"/>
<pin name="O8" direction="oc" function="dot"/>
<pin name="O9" direction="oc" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="7446">
<pin name="IB" direction="in"/>
<pin name="IC" direction="in"/>
<pin name="LT" direction="in" function="dot"/>
<pin name="BI/RBO" direction="in" function="dot"/>
<pin name="RBI" direction="in" function="dot"/>
<pin name="ID" direction="in"/>
<pin name="IA" direction="in"/>
<pin name="E" direction="oc" function="dot"/>
<pin name="D" direction="oc" function="dot"/>
<pin name="C" direction="oc" function="dot"/>
<pin name="B" direction="oc" function="dot"/>
<pin name="A" direction="oc" function="dot"/>
<pin name="G" direction="oc" function="dot"/>
<pin name="F" direction="oc" function="dot"/>
</symbol>
<symbol name="7448">
<pin name="IB" direction="in"/>
<pin name="IC" direction="in"/>
<pin name="LT" direction="in" function="dot"/>
<pin name="BI/RBO" direction="in" function="dot"/>
<pin name="RBI" direction="in" function="dot"/>
<pin name="ID" direction="in"/>
<pin name="IA" direction="in"/>
<pin name="E" direction="out"/>
<pin name="D" direction="out"/>
<pin name="C" direction="out"/>
<pin name="B" direction="out"/>
<pin name="A" direction="out"/>
<pin name="G" direction="out"/>
<pin name="F" direction="out"/>
</symbol>
<symbol name="7449">
<pin name="IB" direction="in"/>
<pin name="IC" direction="in"/>
<pin name="BI" direction="in" function="dot"/>
<pin name="ID" direction="in"/>
<pin name="IA" direction="in"/>
<pin name="E" direction="oc"/>
<pin name="D" direction="oc"/>
<pin name="C" direction="oc"/>
<pin name="B" direction="oc"/>
<pin name="A" direction="oc"/>
<pin name="G" direction="oc"/>
<pin name="F" direction="oc"/>
</symbol>
<symbol name="7450">
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2C" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Y" direction="out" function="dot"/>
<pin name="1Y" direction="out" function="dot"/>
<pin name="1C" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="1X" direction="in"/>
<pin name="!1X" direction="in"/>
<pin name="1B" direction="in"/>
</symbol>
<symbol name="7451">
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2C" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Y" direction="out" function="dot"/>
<pin name="1Y" direction="out" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="1E" direction="in"/>
<pin name="1F" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1C" direction="in"/>
</symbol>
<symbol name="7454">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="Y" direction="out" function="dot"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="I" direction="in"/>
<pin name="J" direction="in"/>
</symbol>
<symbol name="7455">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="Y" direction="out" function="dot"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
</symbol>
<symbol name="7456">
<pin name="CKB" direction="in" function="clk"/>
<pin name="QA" direction="out"/>
<pin name="CKA" direction="in" function="clk"/>
<pin name="CLR" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
</symbol>
<symbol name="7463">
<pin name="I" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7468">
<pin name="1CLKA" direction="in" function="clk"/>
<pin name="1QB" direction="out"/>
<pin name="1QD" direction="out"/>
<pin name="1CLR" direction="in" function="dot"/>
<pin name="2QC" direction="out"/>
<pin name="2QA" direction="out"/>
<pin name="2CLK" direction="in" function="clk"/>
<pin name="2QB" direction="out"/>
<pin name="2CLR" direction="in" function="dot"/>
<pin name="2QD" direction="out"/>
<pin name="1QC" direction="out"/>
<pin name="1QA" direction="out"/>
<pin name="1CLKB" direction="in" function="clk"/>
</symbol>
<symbol name="7470">
<pin name="CLR" direction="in" function="dot"/>
<pin name="J1" direction="in"/>
<pin name="J2" direction="in"/>
<pin name="J" direction="in" function="dot"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="K" direction="in" function="dot"/>
<pin name="K1" direction="in"/>
<pin name="K2" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="PRE" direction="in" function="dot"/>
</symbol>
<symbol name="7472">
<pin name="CLR" direction="in" function="dot"/>
<pin name="J1" direction="in"/>
<pin name="J2" direction="in"/>
<pin name="J3" direction="in"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="K1" direction="in"/>
<pin name="K2" direction="in"/>
<pin name="K3" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="PRE" direction="in" function="dot"/>
</symbol>
<symbol name="7473">
<pin name="CLK" direction="in" function="clk"/>
<pin name="CL" direction="in" function="dot"/>
<pin name="K" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="J" direction="in"/>
</symbol>
<symbol name="7474">
<pin name="CLR" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="7475">
<pin name="!Q1" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="C34" direction="in" function="clk"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="!Q4" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="!Q3" direction="out"/>
<pin name="C12" direction="in" function="clk"/>
<pin name="!Q2" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q1" direction="out"/>
</symbol>
<symbol name="7476">
<pin name="CLK" direction="in" function="clk"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="J" direction="in"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="K" direction="in"/>
</symbol>
<symbol name="7477">
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="34C" direction="in" function="clk"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="4Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="12C" direction="in" function="clk"/>
<pin name="2Q" direction="out"/>
<pin name="1Q" direction="out"/>
</symbol>
<symbol name="7478">
<pin name="CLK" direction="in" function="clk"/>
<pin name="PR1" direction="in" function="dot"/>
<pin name="J1" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="PR2" direction="in" function="dot"/>
<pin name="K2" direction="in"/>
<pin name="Q2" direction="out"/>
<pin name="!Q2" direction="out"/>
<pin name="J2" direction="in"/>
<pin name="!Q1" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="K1" direction="in"/>
</symbol>
<symbol name="7482">
<pin name="S1" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="C0" direction="in"/>
<pin name="C2" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="B2" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="7483">
<pin name="A4" direction="in"/>
<pin name="S3" direction="out"/>
<pin name="A3" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="S2" direction="out"/>
<pin name="B2" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="S1" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="C0" direction="in"/>
<pin name="C4" direction="out"/>
<pin name="S4" direction="out"/>
<pin name="B4" direction="in"/>
</symbol>
<symbol name="7485">
<pin name="B3" direction="in"/>
<pin name="A&lt;B_I" direction="in"/>
<pin name="A=B_I" direction="in"/>
<pin name="A&gt;B_I" direction="in"/>
<pin name="A&gt;B_O" direction="out"/>
<pin name="A=B_O" direction="out"/>
<pin name="A&lt;B_O" direction="out"/>
<pin name="B0" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A3" direction="in"/>
</symbol>
<symbol name="7490">
<pin name="CKB" direction="in" function="clk"/>
<pin name="R0(1)" direction="in"/>
<pin name="R0(2)" direction="in"/>
<pin name="R9(1)" direction="in"/>
<pin name="R9(2)" direction="in"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CKA" direction="in" function="clk"/>
</symbol>
<symbol name="7491">
<pin name="CLK" direction="in" function="clk"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QH" direction="out"/>
<pin name="!QH" direction="out"/>
</symbol>
<symbol name="7492">
<pin name="CKB" direction="in" function="clk"/>
<pin name="R0(1)" direction="in"/>
<pin name="R0(2)" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CKA" direction="in" function="clk"/>
</symbol>
<symbol name="7493">
<pin name="CKB" direction="in" function="clk"/>
<pin name="R0(1)" direction="in"/>
<pin name="R0(2)" direction="in"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CKA" direction="in" function="clk"/>
</symbol>
<symbol name="7495">
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="MOD" direction="in"/>
<pin name="CK2" direction="in" function="clk"/>
<pin name="CK1" direction="in" function="clk"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
</symbol>
<symbol name="7496">
<pin name="CLK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="SER" direction="in"/>
<pin name="QE" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="7497">
<pin name="B1" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="Z" direction="out"/>
<pin name="Y" direction="out"/>
<pin name="EO" direction="out" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="STR" direction="in" function="dot"/>
<pin name="EI" direction="in" function="dot"/>
<pin name="U/C" direction="in" function="dot"/>
<pin name="CLR" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
</symbol>
<symbol name="74100">
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="Q2" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="74107">
<pin name="J" direction="in"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="K" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="74109">
<pin name="CLR" direction="in" function="dot"/>
<pin name="J" direction="in"/>
<pin name="K" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="74111">
<pin name="K" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="J" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="74112">
<pin name="CLK" direction="in" function="clk"/>
<pin name="K" direction="in"/>
<pin name="J" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="74113">
<pin name="CLK" direction="in" function="clk"/>
<pin name="K" direction="in"/>
<pin name="J" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="74114">
<pin name="K" direction="in"/>
<pin name="J" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="74116">
<pin name="CLR" direction="in" function="dot"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="D1" direction="in"/>
<pin name="Q1" direction="out"/>
<pin name="D2" direction="in"/>
<pin name="Q2" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="Q3" direction="out"/>
<pin name="D4" direction="in"/>
<pin name="Q4" direction="out"/>
</symbol>
<symbol name="74120">
<pin name="M" direction="in" function="dot"/>
<pin name="S1" direction="in" function="dot"/>
<pin name="S2" direction="in" function="dot"/>
<pin name="R" direction="in" function="dot"/>
<pin name="C" direction="in" function="dot"/>
<pin name="Y" direction="out"/>
<pin name="!Y" direction="out"/>
</symbol>
<symbol name="74121">
<pin name="!Q" direction="out"/>
<pin name="A1" direction="in" function="dot"/>
<pin name="A2" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="R" direction="in"/>
<pin name="C" direction="in"/>
<pin name="R/C" direction="in"/>
</symbol>
<symbol name="74122">
<pin name="A1" direction="in" function="dot"/>
<pin name="A2" direction="in" function="dot"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="R" direction="in"/>
<pin name="C" direction="in"/>
<pin name="R/C" direction="in"/>
</symbol>
<symbol name="74123">
<pin name="A" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="C" direction="in"/>
<pin name="R/C" direction="in"/>
</symbol>
<symbol name="74124">
<pin name="FC" direction="in"/>
<pin name="RNG" direction="in"/>
<pin name="CX@1" direction="in"/>
<pin name="CX@2" direction="in"/>
<pin name="EN" direction="in" function="dot"/>
<pin name="Y" direction="out" function="dot"/>
</symbol>
<symbol name="74131">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="G1" direction="in"/>
<pin name="Y7" direction="out" function="dot"/>
<pin name="Y6" direction="out" function="dot"/>
<pin name="Y5" direction="out" function="dot"/>
<pin name="Y4" direction="out" function="dot"/>
<pin name="Y3" direction="out" function="dot"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="Y1" direction="out" function="dot"/>
<pin name="Y0" direction="out" function="dot"/>
</symbol>
<symbol name="74137">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="GL" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="G1" direction="in"/>
<pin name="Y7" direction="out" function="dot"/>
<pin name="Y6" direction="out" function="dot"/>
<pin name="Y5" direction="out" function="dot"/>
<pin name="Y4" direction="out" function="dot"/>
<pin name="Y3" direction="out" function="dot"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="Y1" direction="out" function="dot"/>
<pin name="Y0" direction="out" function="dot"/>
</symbol>
<symbol name="74138">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="G2A" direction="in" function="dot"/>
<pin name="G2B" direction="in" function="dot"/>
<pin name="G1" direction="in"/>
<pin name="Y7" direction="out" function="dot"/>
<pin name="Y6" direction="out" function="dot"/>
<pin name="Y5" direction="out" function="dot"/>
<pin name="Y4" direction="out" function="dot"/>
<pin name="Y3" direction="out" function="dot"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="Y1" direction="out" function="dot"/>
<pin name="Y0" direction="out" function="dot"/>
</symbol>
<symbol name="74139">
<pin name="G" direction="in" function="dot"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y0" direction="out" function="dot"/>
<pin name="Y1" direction="out" function="dot"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="Y3" direction="out" function="dot"/>
</symbol>
<symbol name="74143">
<pin name="SCEI" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="RBI" direction="in" function="dot"/>
<pin name="BI" direction="in"/>
<pin name="BI/RBO" function="dot"/>
<pin name="DPI" direction="in"/>
<pin name="DP@2" direction="oc" function="dot"/>
<pin name="D" direction="oc" function="dot"/>
<pin name="F" direction="oc" function="dot"/>
<pin name="E" direction="oc" function="dot"/>
<pin name="G" direction="oc" function="dot"/>
<pin name="C" direction="oc" function="dot"/>
<pin name="A" direction="oc" function="dot"/>
<pin name="B" direction="oc" function="dot"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="STR" direction="in" function="dot"/>
<pin name="DPO" direction="out" function="dot"/>
<pin name="PCEI" direction="in"/>
</symbol>
<symbol name="74145">
<pin name="0" direction="out" function="dot"/>
<pin name="1" direction="out" function="dot"/>
<pin name="2" direction="out" function="dot"/>
<pin name="3" direction="out" function="dot"/>
<pin name="4" direction="out" function="dot"/>
<pin name="5" direction="out" function="dot"/>
<pin name="6" direction="out" function="dot"/>
<pin name="7" direction="out" function="dot"/>
<pin name="8" direction="out" function="dot"/>
<pin name="9" direction="out" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74147">
<pin name="4" direction="in" function="dot"/>
<pin name="5" direction="in" function="dot"/>
<pin name="6" direction="in" function="dot"/>
<pin name="7" direction="in" function="dot"/>
<pin name="8" direction="in" function="dot"/>
<pin name="C" direction="out" function="dot"/>
<pin name="B" direction="out" function="dot"/>
<pin name="A" direction="out" function="dot"/>
<pin name="9" direction="in" function="dot"/>
<pin name="1" direction="in" function="dot"/>
<pin name="2" direction="in" function="dot"/>
<pin name="3" direction="in" function="dot"/>
<pin name="D" direction="out" function="dot"/>
</symbol>
<symbol name="74148">
<pin name="4" direction="in" function="dot"/>
<pin name="5" direction="in" function="dot"/>
<pin name="6" direction="in" function="dot"/>
<pin name="7" direction="in" function="dot"/>
<pin name="EI" direction="in" function="dot"/>
<pin name="A2" direction="out" function="dot"/>
<pin name="A1" direction="out" function="dot"/>
<pin name="A0" direction="out" function="dot"/>
<pin name="0" direction="in" function="dot"/>
<pin name="1" direction="in" function="dot"/>
<pin name="2" direction="in" function="dot"/>
<pin name="3" direction="in" function="dot"/>
<pin name="GS" direction="out" function="dot"/>
<pin name="EO" direction="out"/>
</symbol>
<symbol name="74150">
<pin name="E7" direction="in"/>
<pin name="E6" direction="in"/>
<pin name="E5" direction="in"/>
<pin name="E4" direction="in"/>
<pin name="E3" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="E1" direction="in"/>
<pin name="E0" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="W" direction="out" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="E15" direction="in"/>
<pin name="E14" direction="in"/>
<pin name="E13" direction="in"/>
<pin name="E12" direction="in"/>
<pin name="E11" direction="in"/>
<pin name="E10" direction="in"/>
<pin name="E9" direction="in"/>
<pin name="E8" direction="in"/>
</symbol>
<symbol name="74151">
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="W" direction="out" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
</symbol>
<symbol name="74152">
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="W" direction="out" function="dot"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
</symbol>
<symbol name="74153">
<pin name="1G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="2C0" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C3" direction="in"/>
<pin name="A" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
</symbol>
<symbol name="74154">
<pin name="0" direction="out" function="dot"/>
<pin name="1" direction="out" function="dot"/>
<pin name="2" direction="out" function="dot"/>
<pin name="3" direction="out" function="dot"/>
<pin name="4" direction="out" function="dot"/>
<pin name="5" direction="out" function="dot"/>
<pin name="6" direction="out" function="dot"/>
<pin name="7" direction="out" function="dot"/>
<pin name="8" direction="out" function="dot"/>
<pin name="9" direction="out" function="dot"/>
<pin name="10" direction="out" function="dot"/>
<pin name="11" direction="out" function="dot"/>
<pin name="12" direction="out" function="dot"/>
<pin name="13" direction="out" function="dot"/>
<pin name="14" direction="out" function="dot"/>
<pin name="15" direction="out" function="dot"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74155">
<pin name="1C" direction="in"/>
<pin name="1G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="1Y3" direction="out" function="dot"/>
<pin name="1Y2" direction="out" function="dot"/>
<pin name="1Y1" direction="out" function="dot"/>
<pin name="1Y0" direction="out" function="dot"/>
<pin name="2Y0" direction="out" function="dot"/>
<pin name="2Y1" direction="out" function="dot"/>
<pin name="2Y2" direction="out" function="dot"/>
<pin name="2Y3" direction="out" function="dot"/>
<pin name="A" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2C" direction="in" function="dot"/>
</symbol>
<symbol name="74156">
<pin name="1C" direction="in"/>
<pin name="1G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="1Y3" direction="oc" function="dot"/>
<pin name="1Y2" direction="oc" function="dot"/>
<pin name="1Y1" direction="oc" function="dot"/>
<pin name="1Y0" direction="oc" function="dot"/>
<pin name="2Y0" direction="oc" function="dot"/>
<pin name="2Y1" direction="oc" function="dot"/>
<pin name="2Y2" direction="oc" function="dot"/>
<pin name="2Y3" direction="oc" function="dot"/>
<pin name="A" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
<pin name="2C" direction="in" function="dot"/>
</symbol>
<symbol name="74157">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74158">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out" function="dot"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out" function="dot"/>
<pin name="3Y" direction="out" function="dot"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4Y" direction="out" function="dot"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74159">
<pin name="0" direction="oc" function="dot"/>
<pin name="1" direction="oc" function="dot"/>
<pin name="2" direction="oc" function="dot"/>
<pin name="3" direction="oc" function="dot"/>
<pin name="4" direction="oc" function="dot"/>
<pin name="5" direction="oc" function="dot"/>
<pin name="6" direction="oc" function="dot"/>
<pin name="7" direction="oc" function="dot"/>
<pin name="8" direction="oc" function="dot"/>
<pin name="9" direction="oc" function="dot"/>
<pin name="10" direction="oc" function="dot"/>
<pin name="11" direction="oc" function="dot"/>
<pin name="12" direction="oc" function="dot"/>
<pin name="13" direction="oc" function="dot"/>
<pin name="14" direction="oc" function="dot"/>
<pin name="15" direction="oc" function="dot"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74160">
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="LD" direction="in" function="dot"/>
<pin name="ENT" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="74164">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="QE" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QH" direction="out"/>
</symbol>
<symbol name="74165">
<pin name="SH/!LD" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="!QH" direction="out"/>
<pin name="QH" direction="out"/>
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="INH" direction="in" function="clk"/>
</symbol>
<symbol name="74166">
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="INH" direction="in" function="clk"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="QH" direction="out"/>
<pin name="H" direction="in"/>
<pin name="SH/!LD" direction="in"/>
</symbol>
<symbol name="74167">
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="ST9" direction="in"/>
<pin name="Z" direction="out"/>
<pin name="Y" direction="out"/>
<pin name="EO" direction="out" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="STR" direction="in" function="dot"/>
<pin name="EI" direction="in" function="dot"/>
<pin name="U/C" direction="in" function="dot"/>
<pin name="CLR" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="B1" direction="in"/>
</symbol>
<symbol name="74168">
<pin name="U/!D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="ENP" direction="in" function="dot"/>
<pin name="LD" direction="in" function="dot"/>
<pin name="ENT" direction="in" function="dot"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="RCO" direction="out" function="dot"/>
</symbol>
<symbol name="74170">
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="RB" direction="in"/>
<pin name="RA" direction="in"/>
<pin name="Q4" direction="oc"/>
<pin name="Q3" direction="oc"/>
<pin name="Q2" direction="oc"/>
<pin name="Q1" direction="oc"/>
<pin name="GR" direction="in" function="dot"/>
<pin name="GW" direction="in" function="dot"/>
<pin name="WB" direction="in"/>
<pin name="WA" direction="in"/>
<pin name="D1" direction="in"/>
</symbol>
<symbol name="74171">
<pin name="!Q1" direction="out"/>
<pin name="!Q2" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="Q3" direction="out"/>
<pin name="!Q3" direction="out"/>
<pin name="!Q4" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="D4" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="D1" direction="in"/>
<pin name="Q1" direction="out"/>
</symbol>
<symbol name="74173">
<pin name="M" direction="in" function="dot"/>
<pin name="N" direction="in" function="dot"/>
<pin name="Q1" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q4" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="CLR" direction="in"/>
</symbol>
<symbol name="74174">
<pin name="CLR" direction="in" function="dot"/>
<pin name="Q1" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="Q2" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="Q3" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="Q4" direction="out"/>
<pin name="D4" direction="in"/>
<pin name="Q5" direction="out"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="Q6" direction="out"/>
</symbol>
<symbol name="74175">
<pin name="CLR" direction="in" function="dot"/>
<pin name="Q1" direction="out"/>
<pin name="!Q1" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="!Q2" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="Q3" direction="out"/>
<pin name="!Q3" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="!Q4" direction="out"/>
<pin name="Q4" direction="out"/>
</symbol>
<symbol name="74176">
<pin name="LD" direction="in" function="dot"/>
<pin name="QC" direction="out"/>
<pin name="C" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="CK2" direction="in" function="clk"/>
<pin name="CK1" direction="in" function="clk"/>
<pin name="QB" direction="out"/>
<pin name="B" direction="in"/>
<pin name="D" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="74178">
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="LD" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="SHF" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="74179">
<pin name="CLR" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="LD" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="!QD" direction="out"/>
<pin name="SHF" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="74180">
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="EI" direction="in"/>
<pin name="OI" direction="in"/>
<pin name="EVN" direction="out"/>
<pin name="ODD" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
</symbol>
<symbol name="74181">
<pin name="B0" direction="in" function="dot"/>
<pin name="A0" direction="in" function="dot"/>
<pin name="S3" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="CN" direction="in"/>
<pin name="M" direction="in"/>
<pin name="F0" direction="out" function="dot"/>
<pin name="F1" direction="out" function="dot"/>
<pin name="F2" direction="out" function="dot"/>
<pin name="F3" direction="out" function="dot"/>
<pin name="A=B" direction="out"/>
<pin name="P" direction="out" function="dot"/>
<pin name="CN+4" direction="out"/>
<pin name="G" direction="out" function="dot"/>
<pin name="B3" direction="in" function="dot"/>
<pin name="A3" direction="in" function="dot"/>
<pin name="B2" direction="in" function="dot"/>
<pin name="A2" direction="in" function="dot"/>
<pin name="B1" direction="in" function="dot"/>
<pin name="A1" direction="in" function="dot"/>
</symbol>
<symbol name="74182">
<pin name="G1" direction="in" function="dot"/>
<pin name="P1" direction="in" function="dot"/>
<pin name="G0" direction="in" function="dot"/>
<pin name="P0" direction="in" function="dot"/>
<pin name="G3" direction="in" function="dot"/>
<pin name="P3" direction="in" function="dot"/>
<pin name="P" direction="out" function="dot"/>
<pin name="CN+Z" direction="out"/>
<pin name="G" direction="out" function="dot"/>
<pin name="CN+Y" direction="out"/>
<pin name="CN+X" direction="out"/>
<pin name="CN" direction="in"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="P2" direction="in" function="dot"/>
</symbol>
<symbol name="74183">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="CN" direction="in"/>
<pin name="CN+1" direction="out"/>
<pin name="S" direction="out"/>
</symbol>
<symbol name="74184">
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74190">
<pin name="B" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CTE" direction="in" function="dot"/>
<pin name="D/!U" direction="in"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="LD" direction="in" function="dot"/>
<pin name="MX/MN" direction="out"/>
<pin name="RCO" direction="out" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74192">
<pin name="B" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="DN" direction="in"/>
<pin name="UP" direction="in"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="LD" direction="in" function="dot"/>
<pin name="CO" direction="out" function="dot"/>
<pin name="BO" direction="out" function="dot"/>
<pin name="CLR" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74194">
<pin name="CLR" direction="in" function="dot"/>
<pin name="SR" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="SL" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
</symbol>
<symbol name="74195">
<pin name="CLR" direction="in" function="dot"/>
<pin name="J" direction="in"/>
<pin name="K" direction="in" function="dot"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="S/!L" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="!QD" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
</symbol>
<symbol name="74198">
<pin name="S0" direction="in"/>
<pin name="SR" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="B" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="C" direction="in"/>
<pin name="QC" direction="out"/>
<pin name="D" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="QE" direction="out"/>
<pin name="E" direction="in"/>
<pin name="QF" direction="out"/>
<pin name="F" direction="in"/>
<pin name="QG" direction="out"/>
<pin name="G" direction="in"/>
<pin name="QH" direction="out"/>
<pin name="H" direction="in"/>
<pin name="SL" direction="in"/>
<pin name="S1" direction="in"/>
</symbol>
<symbol name="74199">
<pin name="K" direction="in" function="dot"/>
<pin name="J" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="B" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="C" direction="in"/>
<pin name="QC" direction="out"/>
<pin name="D" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="CINH" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="QE" direction="out"/>
<pin name="E" direction="in"/>
<pin name="QF" direction="out"/>
<pin name="F" direction="in"/>
<pin name="QG" direction="out"/>
<pin name="G" direction="in"/>
<pin name="QH" direction="out"/>
<pin name="H" direction="in"/>
<pin name="SH/!LD" direction="in"/>
</symbol>
<symbol name="74240">
<pin name="G" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="hiz" function="dot"/>
<pin name="Y3" direction="hiz" function="dot"/>
<pin name="Y2" direction="hiz" function="dot"/>
<pin name="Y1" direction="hiz" function="dot"/>
</symbol>
<symbol name="74241">
<pin name="G" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="74242">
<pin name="GAB" direction="in" function="dot"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="B4" function="dot"/>
<pin name="B3" function="dot"/>
<pin name="B2" function="dot"/>
<pin name="B1" function="dot"/>
<pin name="GBA" direction="in"/>
</symbol>
<symbol name="74244">
<pin name="G" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="74245">
<pin name="DIR" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74250">
<pin name="E7" direction="in"/>
<pin name="E6" direction="in"/>
<pin name="E5" direction="in"/>
<pin name="E4" direction="in"/>
<pin name="E3" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="E1" direction="in"/>
<pin name="E0" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="W" direction="hiz" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="E15" direction="in"/>
<pin name="E14" direction="in"/>
<pin name="E13" direction="in"/>
<pin name="E12" direction="in"/>
<pin name="E11" direction="in"/>
<pin name="E10" direction="in"/>
<pin name="E9" direction="in"/>
<pin name="E8" direction="in"/>
</symbol>
<symbol name="74251">
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="Y" direction="hiz"/>
<pin name="W" direction="hiz" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
</symbol>
<symbol name="74253">
<pin name="1G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2Y" direction="hiz"/>
<pin name="2C0" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C3" direction="in"/>
<pin name="A" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
</symbol>
<symbol name="74257">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="hiz"/>
<pin name="3Y" direction="hiz"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4Y" direction="hiz"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74258">
<pin name="!A!/B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="hiz" function="dot"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="hiz" function="dot"/>
<pin name="3Y" direction="hiz" function="dot"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4Y" direction="hiz" function="dot"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74259">
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="D" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="74261">
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="C" direction="in"/>
<pin name="M2" direction="in"/>
<pin name="Q4" direction="out" function="dot"/>
<pin name="Q3" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q0" direction="out"/>
<pin name="M0" direction="in"/>
<pin name="M1" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
</symbol>
<symbol name="74273">
<pin name="CLR" direction="in" function="dot"/>
<pin name="Q1" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="Q4" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="Q5" direction="out"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="Q8" direction="out"/>
</symbol>
<symbol name="74276">
<pin name="CLR" direction="in" function="dot"/>
<pin name="1J" direction="in"/>
<pin name="1CK" direction="in" function="clk"/>
<pin name="1K" direction="in" function="dot"/>
<pin name="1Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="2K" direction="in" function="dot"/>
<pin name="2CK" direction="in" function="clk"/>
<pin name="2J" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="3J" direction="in"/>
<pin name="3CK" direction="in" function="clk"/>
<pin name="3K" direction="in" function="dot"/>
<pin name="3Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="4K" direction="in" function="dot"/>
<pin name="4CK" direction="in" function="clk"/>
<pin name="4J" direction="in"/>
</symbol>
<symbol name="74278">
<pin name="STR" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="P0" direction="in" function="dot"/>
<pin name="P1" direction="out" function="dot"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
</symbol>
<symbol name="74279A">
<pin name="R" direction="in" function="dot"/>
<pin name="S1" direction="in" function="dot"/>
<pin name="S2" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="74280">
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="I" direction="in"/>
<pin name="SEV" direction="out"/>
<pin name="SOD" direction="out" function="dot"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
</symbol>
<symbol name="74283">
<pin name="S2" direction="out"/>
<pin name="B2" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="S1" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="C0" direction="in"/>
<pin name="C4" direction="out"/>
<pin name="S4" direction="out"/>
<pin name="B4" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="S3" direction="out"/>
<pin name="A3" direction="in"/>
<pin name="B3" direction="in"/>
</symbol>
<symbol name="74284">
<pin name="2C" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1C" direction="in"/>
<pin name="Y7" direction="oc"/>
<pin name="Y6" direction="oc"/>
<pin name="Y5" direction="oc"/>
<pin name="Y4" direction="oc"/>
<pin name="GB" direction="in" function="dot"/>
<pin name="GA" direction="in" function="dot"/>
<pin name="2D" direction="in"/>
</symbol>
<symbol name="74285">
<pin name="2C" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1C" direction="in"/>
<pin name="Y3" direction="oc"/>
<pin name="Y2" direction="oc"/>
<pin name="Y1" direction="oc"/>
<pin name="Y0" direction="oc"/>
<pin name="GB" direction="in" function="dot"/>
<pin name="GA" direction="in" function="dot"/>
<pin name="2D" direction="in"/>
</symbol>
<symbol name="74286">
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="XMIT" direction="in" function="dot"/>
<pin name="I" direction="in"/>
<pin name="PAR_ERR" direction="out" function="dot"/>
<pin name="PAR_I/O"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
</symbol>
<symbol name="74290">
<pin name="R9(1)" direction="in"/>
<pin name="R9(2)" direction="in"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="A" direction="in" function="clk"/>
<pin name="B" direction="in" function="clk"/>
<pin name="R0(1)" direction="in"/>
<pin name="R0(2)" direction="in"/>
</symbol>
<symbol name="74292">
<pin name="B" direction="in"/>
<pin name="E" direction="in"/>
<pin name="TP1" direction="out"/>
<pin name="CK1" direction="in" function="clk"/>
<pin name="CK2" direction="in" function="clk"/>
<pin name="TP2" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="A" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="TP3" direction="out"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="74293">
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="A" direction="in" function="clk"/>
<pin name="B" direction="in" function="clk"/>
<pin name="R0(1)" direction="in"/>
<pin name="R0(2)" direction="in"/>
</symbol>
<symbol name="74294">
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="TP" direction="out"/>
<pin name="CK1" direction="in" function="clk"/>
<pin name="CK2" direction="in" function="clk"/>
<pin name="Q" direction="out"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="74295">
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="LD/!SH" direction="in"/>
<pin name="OC" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
</symbol>
<symbol name="74298">
<pin name="B2" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="C2" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="C1" direction="in"/>
<pin name="WS" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
</symbol>
<symbol name="74299">
<pin name="S0" direction="in"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="G/QG"/>
<pin name="E/QE"/>
<pin name="C/QC"/>
<pin name="A/QA"/>
<pin name="QA*" direction="out"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="SR" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="B/QB"/>
<pin name="D/QD"/>
<pin name="F/QF"/>
<pin name="H/QH"/>
<pin name="QH*" direction="out"/>
<pin name="SL" direction="in"/>
<pin name="S1" direction="in"/>
</symbol>
<symbol name="74320">
<pin name="TK1" direction="in"/>
<pin name="TK2" direction="in"/>
<pin name="FFQ" direction="out"/>
<pin name="FFD" direction="in"/>
<pin name="F" direction="out"/>
<pin name="!F*" direction="out"/>
<pin name="F*" direction="out"/>
<pin name="!F" direction="out"/>
<pin name="XTL@1" direction="in"/>
<pin name="XTL@2" direction="in"/>
</symbol>
<symbol name="74321">
<pin name="TK1" direction="in"/>
<pin name="TK2" direction="in"/>
<pin name="FFQ" direction="out"/>
<pin name="FFD" direction="in"/>
<pin name="F/4" direction="out"/>
<pin name="F" direction="out"/>
<pin name="!F*" direction="out"/>
<pin name="F*" direction="out"/>
<pin name="!F" direction="out"/>
<pin name="F/2" direction="out"/>
<pin name="XTL@1" direction="in"/>
<pin name="XTL@2" direction="in"/>
</symbol>
<symbol name="74322">
<pin name="G" direction="in" function="dot"/>
<pin name="S/!P" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="A/QA"/>
<pin name="C/QC" direction="in"/>
<pin name="E/QE" direction="in"/>
<pin name="G/QG"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QH*" direction="hiz"/>
<pin name="H/QH"/>
<pin name="F/QF"/>
<pin name="D/QD" direction="in"/>
<pin name="B/QB"/>
<pin name="D1" direction="in"/>
<pin name="SE" direction="in" function="dot"/>
<pin name="DS" direction="in"/>
</symbol>
<symbol name="74348">
<pin name="4" direction="in" function="dot"/>
<pin name="5" direction="in" function="dot"/>
<pin name="6" direction="in" function="dot"/>
<pin name="7" direction="in" function="dot"/>
<pin name="EI" direction="in"/>
<pin name="A2" direction="hiz" function="dot"/>
<pin name="A1" direction="hiz" function="dot"/>
<pin name="A0" direction="hiz" function="dot"/>
<pin name="0" direction="in" function="dot"/>
<pin name="1" direction="in" function="dot"/>
<pin name="2" direction="in" function="dot"/>
<pin name="3" direction="in" function="dot"/>
<pin name="GS" direction="hiz" function="dot"/>
<pin name="E0" direction="out"/>
</symbol>
<symbol name="74352">
<pin name="1G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
<pin name="1Y" direction="out" function="dot"/>
<pin name="2Y" direction="out" function="dot"/>
<pin name="2C0" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C3" direction="in"/>
<pin name="A" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
</symbol>
<symbol name="74353">
<pin name="1G" direction="in" function="dot"/>
<pin name="B" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
<pin name="1Y" direction="hiz" function="dot"/>
<pin name="2Y" direction="hiz" function="dot"/>
<pin name="2C0" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C3" direction="in"/>
<pin name="A" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
</symbol>
<symbol name="74354">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="DC" direction="in" function="dot"/>
<pin name="SC" direction="in" function="dot"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="G3" direction="in"/>
<pin name="W" direction="hiz" function="dot"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="74355">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="DC" direction="in" function="dot"/>
<pin name="SC" direction="in" function="dot"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="G3" direction="in"/>
<pin name="W" direction="oc" function="dot"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="74356">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="SC" direction="in" function="dot"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="G3" direction="in"/>
<pin name="W" direction="hiz" function="dot"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="74357">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="SC" direction="in" function="dot"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="G3" direction="in"/>
<pin name="W" direction="oc" function="dot"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="74365">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="Y1" direction="hiz"/>
<pin name="A2" direction="in"/>
<pin name="Y2" direction="hiz"/>
<pin name="A3" direction="in"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="A4" direction="in"/>
<pin name="Y5" direction="hiz"/>
<pin name="A5" direction="in"/>
<pin name="Y6" direction="hiz"/>
<pin name="A6" direction="in"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74366">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="Y1" direction="hiz" function="dot"/>
<pin name="A2" direction="in"/>
<pin name="Y2" direction="hiz" function="dot"/>
<pin name="A3" direction="in"/>
<pin name="Y3" direction="hiz" function="dot"/>
<pin name="Y4" direction="hiz" function="dot"/>
<pin name="A4" direction="in"/>
<pin name="Y5" direction="hiz" function="dot"/>
<pin name="A5" direction="in"/>
<pin name="Y6" direction="hiz" function="dot"/>
<pin name="A6" direction="in"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74367">
<pin name="1G" direction="in" function="dot"/>
<pin name="1A1" direction="in"/>
<pin name="1Y1" direction="hiz"/>
<pin name="1A2" direction="in"/>
<pin name="1Y2" direction="hiz"/>
<pin name="1A3" direction="in"/>
<pin name="1Y3" direction="hiz"/>
<pin name="1Y4" direction="hiz"/>
<pin name="1A4" direction="in"/>
<pin name="2Y1" direction="hiz"/>
<pin name="2A1" direction="in"/>
<pin name="2Y2" direction="hiz"/>
<pin name="2A2" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
</symbol>
<symbol name="74368">
<pin name="1G" direction="in" function="dot"/>
<pin name="1A1" direction="in"/>
<pin name="1Y1" direction="hiz" function="dot"/>
<pin name="1A2" direction="in"/>
<pin name="1Y2" direction="hiz" function="dot"/>
<pin name="1A3" direction="in"/>
<pin name="1Y3" direction="hiz" function="dot"/>
<pin name="1Y4" direction="hiz" function="dot"/>
<pin name="1A4" direction="in"/>
<pin name="2Y1" direction="hiz" function="dot"/>
<pin name="2A1" direction="in"/>
<pin name="2Y2" direction="hiz" function="dot"/>
<pin name="2A2" direction="in"/>
<pin name="2G" direction="in" function="dot"/>
</symbol>
<symbol name="74373">
<pin name="OC" direction="in" function="dot"/>
<pin name="1Q" direction="hiz"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="4Q" direction="hiz"/>
<pin name="ENC" direction="in"/>
<pin name="5Q" direction="hiz"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="6Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="8Q" direction="hiz"/>
</symbol>
<symbol name="74374">
<pin name="OC" direction="in" function="dot"/>
<pin name="1Q" direction="hiz"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="4Q" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="5Q" direction="hiz"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="6Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="8Q" direction="hiz"/>
</symbol>
<symbol name="74375">
<pin name="1D" direction="in"/>
<pin name="!1Q" direction="out"/>
<pin name="1Q" direction="out"/>
<pin name="12C" direction="in"/>
<pin name="2Q" direction="out"/>
<pin name="!2Q" direction="out"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="!3Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="34C" direction="in"/>
<pin name="4Q" direction="out"/>
<pin name="!4Q" direction="out"/>
<pin name="4D" direction="in"/>
</symbol>
<symbol name="74376">
<pin name="CLR" direction="in" function="dot"/>
<pin name="1J" direction="in"/>
<pin name="1K" direction="in" function="dot"/>
<pin name="1Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="2K" direction="in" function="dot"/>
<pin name="2J" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="3J" direction="in"/>
<pin name="3K" direction="in" function="dot"/>
<pin name="3Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="4K" direction="in" function="dot"/>
<pin name="4J" direction="in"/>
</symbol>
<symbol name="74377">
<pin name="G" direction="in" function="dot"/>
<pin name="1Q" direction="out"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="4Q" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="5Q" direction="out"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="6Q" direction="out"/>
<pin name="7Q" direction="out"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="8Q" direction="out"/>
</symbol>
<symbol name="74378">
<pin name="G" direction="in" function="dot"/>
<pin name="1Q" direction="out"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Q" direction="out"/>
<pin name="3D" direction="in"/>
<pin name="3Q" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="4Q" direction="out"/>
<pin name="4D" direction="in"/>
<pin name="5Q" direction="out"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="6Q" direction="out"/>
</symbol>
<symbol name="74379">
<pin name="G" direction="in" function="dot"/>
<pin name="1Q" direction="out"/>
<pin name="!1Q" direction="out"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="!2Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="3Q" direction="out"/>
<pin name="!3Q" direction="out"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="!4Q" direction="out"/>
<pin name="4Q" direction="out"/>
</symbol>
<symbol name="74381">
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="F0" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="G" direction="out" function="dot"/>
<pin name="P" direction="out" function="dot"/>
<pin name="CN" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="74382">
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="B0" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="F0" direction="out"/>
<pin name="F1" direction="out"/>
<pin name="F2" direction="out"/>
<pin name="F3" direction="out"/>
<pin name="OVR" direction="out"/>
<pin name="CN+4" direction="out"/>
<pin name="CN" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="74384">
<pin name="CLR" direction="in" function="dot"/>
<pin name="X3" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X0" direction="in"/>
<pin name="PRD" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="MOD" direction="in"/>
<pin name="K" direction="in"/>
<pin name="X7" direction="in"/>
<pin name="X6" direction="in"/>
<pin name="X5" direction="in"/>
<pin name="X4" direction="in"/>
<pin name="Y" direction="in"/>
</symbol>
<symbol name="74385">
<pin name="CLK" direction="in" function="clk"/>
<pin name="1S" direction="out"/>
<pin name="1S/!A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2S/!A" direction="in"/>
<pin name="2S" direction="out"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="3S" direction="out"/>
<pin name="3S/!A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="4B" direction="in"/>
<pin name="4S/!A" direction="in"/>
<pin name="4S" direction="out"/>
</symbol>
<symbol name="74390">
<pin name="A" direction="in" function="clk"/>
<pin name="CLR" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="B" direction="in" function="clk"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="74393">
<pin name="A" direction="in" function="clk"/>
<pin name="CLR" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="74395">
<pin name="CLR" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="LD/!SH" direction="in"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QD*" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QB" direction="hiz"/>
<pin name="QA" direction="hiz"/>
</symbol>
<symbol name="74396">
<pin name="2Q1" direction="out"/>
<pin name="1Q1" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="2Q2" direction="out"/>
<pin name="1Q2" direction="out"/>
<pin name="D2" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="D3" direction="in"/>
<pin name="1Q3" direction="out"/>
<pin name="2Q3" direction="out"/>
<pin name="D4" direction="in"/>
<pin name="1Q4" direction="out"/>
<pin name="2Q4" direction="out"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74398">
<pin name="WS" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="!QA" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="!QB" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QC" direction="out"/>
<pin name="!QC" direction="out"/>
<pin name="C1" direction="in"/>
<pin name="C2" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="!QD" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="74399">
<pin name="WS" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QC" direction="out"/>
<pin name="C1" direction="in"/>
<pin name="C2" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="74412">
<pin name="S1" direction="in" function="dot"/>
<pin name="M" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DO1" direction="hiz"/>
<pin name="DI2" direction="in"/>
<pin name="DO2" direction="hiz"/>
<pin name="DI3" direction="in"/>
<pin name="DO3" direction="hiz"/>
<pin name="DI4" direction="in"/>
<pin name="DO4" direction="hiz"/>
<pin name="STB" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="DO5" direction="hiz"/>
<pin name="DI5" direction="in"/>
<pin name="DO6" direction="hiz"/>
<pin name="DI6" direction="in"/>
<pin name="DO7" direction="hiz"/>
<pin name="DI7" direction="in"/>
<pin name="DO8" direction="hiz"/>
<pin name="DI8" direction="in"/>
<pin name="INT" direction="out" function="dot"/>
</symbol>
<symbol name="74422">
<pin name="A1" direction="in" function="dot"/>
<pin name="A2" direction="in" function="dot"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
<pin name="RI" direction="in"/>
<pin name="CX" direction="in"/>
<pin name="RCX" direction="in"/>
</symbol>
<symbol name="74440">
<pin name="CS" direction="in" function="dot"/>
<pin name="B1"/>
<pin name="C1"/>
<pin name="C2"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="C3"/>
<pin name="C4"/>
<pin name="B4"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="GA" direction="in" function="dot"/>
<pin name="GB" direction="in" function="dot"/>
<pin name="GC" direction="in" function="dot"/>
</symbol>
<symbol name="74445">
<pin name="O0" direction="out" function="dot"/>
<pin name="O1" direction="out" function="dot"/>
<pin name="O2" direction="out" function="dot"/>
<pin name="O3" direction="out" function="dot"/>
<pin name="O4" direction="out" function="dot"/>
<pin name="O5" direction="out" function="dot"/>
<pin name="O6" direction="out" function="dot"/>
<pin name="O7" direction="out" function="dot"/>
<pin name="O8" direction="out" function="dot"/>
<pin name="O9" direction="out" function="dot"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74446">
<pin name="GBA" direction="in" function="dot"/>
<pin name="A1"/>
<pin name="DR2" direction="in" function="dot"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="DR3" direction="in" function="dot"/>
<pin name="A4"/>
<pin name="B4"/>
<pin name="DR4" direction="in" function="dot"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="DR1" direction="in" function="dot"/>
<pin name="B1"/>
<pin name="GAB" direction="in" function="dot"/>
</symbol>
<symbol name="74449">
<pin name="GBA" direction="in" function="dot"/>
<pin name="A1"/>
<pin name="DR2" direction="in" function="dot"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="DR3" direction="in" function="dot"/>
<pin name="A4"/>
<pin name="B4"/>
<pin name="DR4" direction="in" function="dot"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="DR1" direction="in" function="dot"/>
<pin name="B1"/>
<pin name="GAB" direction="in" function="dot"/>
</symbol>
<symbol name="74465">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="Y1" direction="hiz"/>
<pin name="A2" direction="in"/>
<pin name="Y2" direction="hiz"/>
<pin name="A3" direction="in"/>
<pin name="Y3" direction="hiz"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="A5" direction="in"/>
<pin name="Y6" direction="hiz"/>
<pin name="A6" direction="in"/>
<pin name="Y7" direction="hiz"/>
<pin name="A7" direction="in"/>
<pin name="Y8" direction="hiz"/>
<pin name="A8" direction="in"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74466">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="Y1" direction="hiz" function="dot"/>
<pin name="A2" direction="in"/>
<pin name="Y2" direction="hiz" function="dot"/>
<pin name="A3" direction="in"/>
<pin name="Y3" direction="hiz" function="dot"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="hiz" function="dot"/>
<pin name="Y5" direction="hiz" function="dot"/>
<pin name="A5" direction="in"/>
<pin name="Y6" direction="hiz" function="dot"/>
<pin name="A6" direction="in"/>
<pin name="Y7" direction="hiz" function="dot"/>
<pin name="A7" direction="in"/>
<pin name="Y8" direction="hiz" function="dot"/>
<pin name="A8" direction="in"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74467">
<pin name="G" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="Y1" direction="hiz"/>
<pin name="A2" direction="in"/>
<pin name="Y2" direction="hiz"/>
<pin name="A3" direction="in"/>
<pin name="Y3" direction="hiz"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="hiz"/>
</symbol>
<symbol name="74468">
<pin name="G" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="Y1" direction="hiz" function="dot"/>
<pin name="A2" direction="in"/>
<pin name="Y2" direction="hiz" function="dot"/>
<pin name="A3" direction="in"/>
<pin name="Y3" direction="hiz" function="dot"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="hiz" function="dot"/>
</symbol>
<symbol name="74490">
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="ST9" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="OSCPWR">
<pin name="OSCGND" direction="pwr"/>
<pin name="OSCVCC" direction="pwr"/>
</symbol>
<symbol name="74279B">
<pin name="R" direction="in" function="dot"/>
<pin name="S" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="74243">
<pin name="GAB" direction="in" function="dot"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="GBA" direction="in"/>
</symbol>
<symbol name="74282">
<pin name="G1" direction="in" function="dot"/>
<pin name="P1" direction="in" function="dot"/>
<pin name="G0" direction="in" function="dot"/>
<pin name="P0" direction="in" function="dot"/>
<pin name="G3" direction="in" function="dot"/>
<pin name="P3" direction="in" function="dot"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="P" direction="out" function="dot"/>
<pin name="CN+Z" direction="out"/>
<pin name="G" direction="out" function="dot"/>
<pin name="CN*" direction="out"/>
<pin name="CN+Y" direction="out"/>
<pin name="CN+X" direction="out"/>
<pin name="CNB" direction="in"/>
<pin name="CNA" direction="in"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="P2" direction="in" function="dot"/>
</symbol>
<symbol name="7434">
<pin name="I" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="74125">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
</symbol>
<symbol name="74126">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7400">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7401">
<pin name="O" direction="oc" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7402">
<pin name="O" direction="out" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7403">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="7408">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7409">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc"/>
</symbol>
<symbol name="7410">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7411">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7412">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7413">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7415">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7421">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7422">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="7425">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="G" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7427">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7430">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
</symbol>
<symbol name="7432">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7433">
<pin name="O" direction="out" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7439">
<pin name="O" direction="oc" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7465">
<pin name="I0" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
<pin name="I9" direction="in"/>
<pin name="I10" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
</symbol>
<symbol name="7486">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="74133">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="I9" direction="in"/>
<pin name="I10" direction="in"/>
<pin name="I11" direction="in"/>
<pin name="I12" direction="in"/>
</symbol>
<symbol name="74134">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="I9" direction="in"/>
<pin name="I10" direction="in"/>
<pin name="I11" direction="in"/>
<pin name="OE" direction="in"/>
</symbol>
<symbol name="74135">
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
</symbol>
<symbol name="74136">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc"/>
</symbol>
<symbol name="74260">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
</symbol>
<symbol name="74266">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="74386">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7420">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7436">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7437">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="74350">
<pin name="OE" direction="in" function="dot"/>
<pin name="S0"/>
<pin name="S1" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D-1" direction="in"/>
<pin name="D-2" direction="in"/>
<pin name="D-3" direction="in"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
<pin name="Y0" direction="hiz"/>
</symbol>
<symbol name="74337">
<pin name="G" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="Y1" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="Q1" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q4" direction="hiz"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
</symbol>
<symbol name="74303">
<pin name="PRE" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out" function="dot"/>
<pin name="Q8" direction="out" function="dot"/>
</symbol>
<symbol name="2PWR3GND">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="74304">
<pin name="PRE" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="Q8" direction="out"/>
</symbol>
<symbol name="2PWR1GND">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="7460">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="X" direction="out"/>
<pin name="!X" direction="out"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="7480">
<pin name="B*"/>
<pin name="BC" direction="in" function="dot"/>
<pin name="CN" direction="in"/>
<pin name="CN+1" direction="out" function="dot"/>
<pin name="S" direction="out"/>
<pin name="!S" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A*"/>
<pin name="AC" direction="in" function="dot"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
</symbol>
<symbol name="7494">
<pin name="P1A" direction="in"/>
<pin name="P1B" direction="in"/>
<pin name="P1C" direction="in"/>
<pin name="P1D" direction="in"/>
<pin name="PE1" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="OUT" direction="out"/>
<pin name="CLR" direction="in"/>
<pin name="P2D" direction="in"/>
<pin name="P2C" direction="in"/>
<pin name="P2B" direction="in"/>
<pin name="PE2" direction="in"/>
<pin name="P2A" direction="in"/>
</symbol>
<symbol name="74104">
<pin name="JK" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="K1" direction="in"/>
<pin name="J1" direction="in"/>
<pin name="J2" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="K2" direction="in"/>
<pin name="K3" direction="in"/>
<pin name="J3" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="74105">
<pin name="JK" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="K1" direction="in"/>
<pin name="J1" direction="in"/>
<pin name="J2" direction="in" function="dot"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="K2" direction="in" function="dot"/>
<pin name="K3" direction="in"/>
<pin name="J3" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
</symbol>
<symbol name="74141">
<pin name="8" direction="oc" function="dot"/>
<pin name="9" direction="oc" function="dot"/>
<pin name="A" direction="in"/>
<pin name="D" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="2" direction="oc" function="dot"/>
<pin name="3" direction="oc" function="dot"/>
<pin name="7" direction="oc" function="dot"/>
<pin name="6" direction="oc" function="dot"/>
<pin name="4" direction="oc" function="dot"/>
<pin name="5" direction="oc" function="dot"/>
<pin name="1" direction="oc" function="dot"/>
<pin name="0" direction="oc" function="dot"/>
</symbol>
<symbol name="74142">
<pin name="CLR" direction="in" function="dot"/>
<pin name="7" direction="oc" function="dot"/>
<pin name="6" direction="oc" function="dot"/>
<pin name="4" direction="oc" function="dot"/>
<pin name="5" direction="oc" function="dot"/>
<pin name="3" direction="oc" function="dot"/>
<pin name="2" direction="oc" function="dot"/>
<pin name="1" direction="oc" function="dot"/>
<pin name="0" direction="oc" function="dot"/>
<pin name="8" direction="oc" function="dot"/>
<pin name="9" direction="oc" function="dot"/>
<pin name="STRB" direction="in" function="dot"/>
<pin name="QD" direction="out" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="74172">
<pin name="1W1" direction="in"/>
<pin name="1W0" direction="in"/>
<pin name="1GW" direction="in" function="dot"/>
<pin name="1DB" direction="in"/>
<pin name="2DB" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="1R2" direction="in"/>
<pin name="1R1" direction="in"/>
<pin name="1R0" direction="in"/>
<pin name="1QB" direction="hiz" function="dot"/>
<pin name="2QB" direction="hiz" function="dot"/>
<pin name="2QA" direction="hiz" function="dot"/>
<pin name="1QA" direction="hiz" function="dot"/>
<pin name="1GR" direction="in" function="dot"/>
<pin name="2GR" direction="in" function="dot"/>
<pin name="2W/R0" direction="in"/>
<pin name="2W/R1" direction="in"/>
<pin name="2W/R2" direction="in"/>
<pin name="2GW" direction="in" function="dot"/>
<pin name="2DA" direction="in"/>
<pin name="1DA" direction="in"/>
<pin name="1W2" direction="in"/>
</symbol>
<symbol name="74226">
<pin name="GBA" direction="in" function="dot"/>
<pin name="S1" direction="in"/>
<pin name="A1" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="A4" direction="hiz"/>
<pin name="OCBA" direction="in"/>
<pin name="OCAB" direction="in"/>
<pin name="B4" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="B1" direction="hiz"/>
<pin name="S2" direction="in"/>
<pin name="GAB" direction="in" function="dot"/>
</symbol>
<symbol name="74268">
<pin name="OC" direction="in" function="dot"/>
<pin name="Q1" direction="hiz"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="Q2" direction="hiz"/>
<pin name="D3" direction="in"/>
<pin name="Q3" direction="hiz"/>
<pin name="C" direction="in"/>
<pin name="Q4" direction="hiz"/>
<pin name="D4" direction="in"/>
<pin name="Q5" direction="hiz"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="Q6" direction="hiz"/>
</symbol>
<symbol name="74274">
<pin name="AN" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AN3" direction="in"/>
<pin name="BN" direction="in"/>
<pin name="N" direction="out"/>
<pin name="N+1" direction="out"/>
<pin name="N+2" direction="out"/>
<pin name="N+3" direction="out"/>
<pin name="N+4" direction="out"/>
<pin name="N+5" direction="out"/>
<pin name="N+6" direction="out"/>
<pin name="N+7" direction="out"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="BN1" direction="in"/>
<pin name="BN2" direction="in"/>
<pin name="BN3" direction="in"/>
</symbol>
<symbol name="74275">
<pin name="2N@1" direction="in"/>
<pin name="2N@2" direction="in"/>
<pin name="2N@3" direction="in"/>
<pin name="2N@4" direction="in"/>
<pin name="C2N@1" direction="in"/>
<pin name="C2N@2" direction="in"/>
<pin name="2N@5" direction="in"/>
<pin name="2N+0" direction="hiz"/>
<pin name="C2N+1" direction="hiz"/>
<pin name="2N+1" direction="hiz"/>
<pin name="2N+2" direction="hiz"/>
<pin name="G" direction="in" function="dot"/>
<pin name="2N@6" direction="in"/>
<pin name="2N@7" direction="in"/>
</symbol>
<symbol name="74428">
<pin name="STSTB" direction="in" function="dot"/>
<pin name="HLDA" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="DBIN" direction="in"/>
<pin name="DB4"/>
<pin name="D4"/>
<pin name="DB7"/>
<pin name="D7"/>
<pin name="DB3"/>
<pin name="D3"/>
<pin name="DB2"/>
<pin name="D2"/>
<pin name="DB0"/>
<pin name="D0"/>
<pin name="DB1"/>
<pin name="D1"/>
<pin name="DB5"/>
<pin name="D5"/>
<pin name="DB6"/>
<pin name="D6"/>
<pin name="BUSEN" direction="in" function="dot"/>
<pin name="INTA" direction="out" function="dot"/>
<pin name="MEMR" direction="out" function="dot"/>
<pin name="I/OR" direction="out" function="dot"/>
<pin name="MEMW" direction="out" function="dot"/>
<pin name="I/OW" direction="out" function="dot"/>
</symbol>
<symbol name="74432">
<pin name="S1" direction="in" function="dot"/>
<pin name="M" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="O1" direction="hiz" function="dot"/>
<pin name="D2" direction="in"/>
<pin name="O2" direction="hiz" function="dot"/>
<pin name="D3" direction="in"/>
<pin name="O3" direction="hiz" function="dot"/>
<pin name="D4" direction="in"/>
<pin name="O4" direction="hiz" function="dot"/>
<pin name="STB" direction="in" function="clk"/>
<pin name="S2" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="O5" direction="hiz" function="dot"/>
<pin name="D5" direction="in"/>
<pin name="O6" direction="hiz" function="dot"/>
<pin name="D6" direction="in"/>
<pin name="O7" direction="hiz" function="dot"/>
<pin name="D7" direction="in"/>
<pin name="O8" direction="hiz" function="dot"/>
<pin name="D8" direction="in"/>
<pin name="INT" direction="out" function="dot"/>
</symbol>
<symbol name="74436">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="Y1" direction="out" function="dot"/>
<pin name="A2" direction="in"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="A3" direction="in"/>
<pin name="Y3" direction="out" function="dot"/>
<pin name="Y4" direction="out" function="dot"/>
<pin name="A4" direction="in"/>
<pin name="Y5" direction="out" function="dot"/>
<pin name="A5" direction="in"/>
<pin name="Y6" direction="out" function="dot"/>
<pin name="A6" direction="in"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74484">
<pin name="E" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y1" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y7" direction="hiz"/>
<pin name="Y8" direction="hiz"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="H" direction="in"/>
<pin name="G" direction="in"/>
<pin name="F" direction="in"/>
</symbol>
<symbol name="7402EU">
<pin name="O" direction="out" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="74135EU">
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="out"/>
</symbol>
<symbol name="74136EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc"/>
</symbol>
<symbol name="74260EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
</symbol>
<symbol name="74266EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="74386EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7425EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="G" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7427EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I2" direction="in"/>
</symbol>
<symbol name="7432EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7433EU">
<pin name="O" direction="out" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7486EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7465EU">
<pin name="O" direction="oc" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="I9" direction="in"/>
<pin name="I10" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
</symbol>
<symbol name="7464EU">
<pin name="O" direction="out" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="I9" direction="in"/>
<pin name="I10" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
</symbol>
<symbol name="7464">
<pin name="I0" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="O" direction="out" function="dot"/>
<pin name="I9" direction="in"/>
<pin name="I10" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
</symbol>
<symbol name="74518">
<pin name="G" direction="in" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="oc"/>
</symbol>
<symbol name="74520">
<pin name="G1" direction="in" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="out" function="dot"/>
</symbol>
<symbol name="74522">
<pin name="G1" direction="in" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="oc" function="dot"/>
</symbol>
<symbol name="74526">
<pin name="G" direction="in" function="dot"/>
<pin name="P0" direction="in" function="dot"/>
<pin name="P1" direction="in" function="dot"/>
<pin name="P2" direction="in" function="dot"/>
<pin name="P3" direction="in" function="dot"/>
<pin name="P4" direction="in" function="dot"/>
<pin name="P5" direction="in" function="dot"/>
<pin name="P6" direction="in" function="dot"/>
<pin name="P7" direction="in" function="dot"/>
<pin name="P8" direction="in" function="dot"/>
<pin name="P9" direction="in" function="dot"/>
<pin name="P10" direction="in" function="dot"/>
<pin name="P11" direction="in" function="dot"/>
<pin name="P12" direction="in" function="dot"/>
<pin name="P13" direction="in" function="dot"/>
<pin name="P14" direction="in" function="dot"/>
<pin name="P15" direction="in" function="dot"/>
<pin name="P=Q" direction="out" function="dot"/>
</symbol>
<symbol name="74527">
<pin name="G" direction="in" function="dot"/>
<pin name="P0" direction="in" function="dot"/>
<pin name="P1" direction="in" function="dot"/>
<pin name="P2" direction="in" function="dot"/>
<pin name="P3" direction="in" function="dot"/>
<pin name="P4" direction="in" function="dot"/>
<pin name="P5" direction="in" function="dot"/>
<pin name="P6" direction="in" function="dot"/>
<pin name="P7" direction="in" function="dot"/>
<pin name="P8" direction="in"/>
<pin name="Q8" direction="in"/>
<pin name="P9" direction="in"/>
<pin name="Q9" direction="in"/>
<pin name="P10" direction="in"/>
<pin name="Q10" direction="in"/>
<pin name="P11" direction="in"/>
<pin name="Q11" direction="in"/>
<pin name="P=Q" direction="out" function="dot"/>
</symbol>
<symbol name="74528">
<pin name="G1" direction="in" function="dot"/>
<pin name="P0" direction="in" function="dot"/>
<pin name="P1" direction="in" function="dot"/>
<pin name="P2" direction="in" function="dot"/>
<pin name="P3" direction="in" function="dot"/>
<pin name="P4" direction="in" function="dot"/>
<pin name="P5" direction="in" function="dot"/>
<pin name="P6" direction="in" function="dot"/>
<pin name="P7" direction="in" function="dot"/>
<pin name="P8" direction="in" function="dot"/>
<pin name="P9" direction="in" function="dot"/>
<pin name="P10" direction="in" function="dot"/>
<pin name="P11" direction="in" function="dot"/>
<pin name="P=Q" direction="out" function="dot"/>
</symbol>
<symbol name="74540">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="Y8" direction="hiz" function="dot"/>
<pin name="Y7" direction="hiz" function="dot"/>
<pin name="Y6" direction="hiz" function="dot"/>
<pin name="Y5" direction="hiz" function="dot"/>
<pin name="Y4" direction="hiz" function="dot"/>
<pin name="Y3" direction="hiz" function="dot"/>
<pin name="Y2" direction="hiz" function="dot"/>
<pin name="Y1" direction="hiz" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74541">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="Y8" direction="hiz"/>
<pin name="Y7" direction="hiz"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74560">
<pin name="ALD" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="ACL" direction="in" function="dot"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SLD" direction="in" function="dot"/>
<pin name="ENT" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="G" direction="in" function="dot"/>
<pin name="CCO" direction="out"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="74568">
<pin name="U/!D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="ENP" direction="in" function="dot"/>
<pin name="ACLR" direction="in" function="dot"/>
<pin name="SCLR" direction="in" function="dot"/>
<pin name="LOAD" direction="in" function="dot"/>
<pin name="ENT" direction="in" function="dot"/>
<pin name="QD" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QB" direction="hiz"/>
<pin name="QA" direction="hiz"/>
<pin name="G" direction="in" function="dot"/>
<pin name="CCO" direction="hiz" function="dot"/>
<pin name="RCO" direction="hiz" function="dot"/>
</symbol>
<symbol name="74589">
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="QH*" direction="hiz"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="SRCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="SRLD" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74590">
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="RCO" direction="out" function="dot"/>
<pin name="CCLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CCKEN" direction="in" function="dot"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="QA" direction="hiz"/>
</symbol>
<symbol name="74591">
<pin name="QB" direction="oc"/>
<pin name="QC" direction="oc"/>
<pin name="QD" direction="oc"/>
<pin name="QE" direction="oc"/>
<pin name="QF" direction="oc"/>
<pin name="QG" direction="oc"/>
<pin name="QH" direction="oc"/>
<pin name="RCO" direction="out" function="dot"/>
<pin name="CCLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CCKEN" direction="in" function="dot"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="QA" direction="oc"/>
</symbol>
<symbol name="74592">
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="RCO" direction="out" function="dot"/>
<pin name="CCL" direction="in" function="dot"/>
<pin name="CCK" direction="in" function="clk"/>
<pin name="CCKEN" direction="in" function="dot"/>
<pin name="RCK" direction="in"/>
<pin name="CLD" direction="in" function="dot"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74593">
<pin name="A/QA"/>
<pin name="B/QB"/>
<pin name="C/QC"/>
<pin name="D/QD"/>
<pin name="E/QE"/>
<pin name="F/QF"/>
<pin name="G/QG"/>
<pin name="H/QH"/>
<pin name="CLOAD" direction="in" function="dot"/>
<pin name="RCO" direction="out" function="dot"/>
<pin name="CCLR" direction="in" function="dot"/>
<pin name="CCK" direction="in" function="clk"/>
<pin name="!CCKEN" direction="in"/>
<pin name="CCKEN" direction="in"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="RCKEN" direction="in" function="dot"/>
<pin name="!G" direction="in"/>
<pin name="G" direction="in"/>
</symbol>
<symbol name="74594">
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QH" direction="out"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="RCL" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QH*" direction="out"/>
</symbol>
<symbol name="74595">
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QH*" direction="hiz"/>
</symbol>
<symbol name="74596">
<pin name="QB" direction="oc"/>
<pin name="QC" direction="oc"/>
<pin name="QD" direction="oc"/>
<pin name="QE" direction="oc"/>
<pin name="QF" direction="oc"/>
<pin name="QG" direction="oc"/>
<pin name="QH" direction="oc"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="oc"/>
<pin name="QH*" direction="oc"/>
</symbol>
<symbol name="74597">
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="QH*" direction="out"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SRCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="SLD" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="74598">
<pin name="A/QA"/>
<pin name="B/QB"/>
<pin name="C/QC"/>
<pin name="D/QD"/>
<pin name="E/QE"/>
<pin name="F/QF"/>
<pin name="G/QG"/>
<pin name="H/QH"/>
<pin name="SLD" direction="in" function="dot"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="SCKE" direction="in" function="dot"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="G" direction="in" function="dot"/>
<pin name="SR1" direction="in"/>
<pin name="SR0" direction="in"/>
<pin name="DS" direction="in"/>
<pin name="QH*"/>
</symbol>
<symbol name="74599">
<pin name="QB" direction="oc"/>
<pin name="QC" direction="oc"/>
<pin name="QD" direction="oc"/>
<pin name="QE" direction="oc"/>
<pin name="QF" direction="oc"/>
<pin name="QG" direction="oc"/>
<pin name="QH" direction="oc"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="RCL" direction="in" function="dot"/>
<pin name="SER" direction="in"/>
<pin name="QA" direction="oc"/>
<pin name="QH*" direction="oc"/>
</symbol>
<symbol name="74604">
<pin name="CLK" direction="in" function="clk"/>
<pin name="A/!B" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y7" direction="hiz"/>
<pin name="Y8" direction="hiz"/>
<pin name="B8" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="A5" direction="in"/>
</symbol>
<symbol name="74605">
<pin name="CLK" direction="in" function="clk"/>
<pin name="A/!B" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="Y4" direction="oc"/>
<pin name="Y3" direction="oc"/>
<pin name="Y2" direction="oc"/>
<pin name="Y1" direction="oc"/>
<pin name="Y5" direction="oc"/>
<pin name="Y6" direction="oc"/>
<pin name="Y7" direction="oc"/>
<pin name="Y8" direction="oc"/>
<pin name="B8" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="A5" direction="in"/>
</symbol>
<symbol name="74608">
<pin name="PRECHRG" direction="in"/>
<pin name="P/!N" direction="in"/>
<pin name="R/!W_I" direction="in"/>
<pin name="R/!W_O" direction="out"/>
<pin name="RAS_EN" direction="in" function="dot"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="CAS/!HLD" direction="in"/>
<pin name="ROW/!COL" direction="out"/>
<pin name="RC_RAH" direction="in"/>
<pin name="START" direction="in" function="clk"/>
<pin name="REFRESH" direction="in"/>
<pin name="RC/CAS" direction="in"/>
<pin name="RMW" direction="in" function="dot"/>
</symbol>
<symbol name="74620">
<pin name="GAB" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B8" direction="hiz"/>
<pin name="B7" direction="hiz"/>
<pin name="B6" direction="hiz"/>
<pin name="B5" direction="hiz"/>
<pin name="B4" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="B1" direction="hiz"/>
<pin name="GBA" direction="in" function="dot"/>
</symbol>
<symbol name="74621">
<pin name="GAB" direction="in"/>
<pin name="A1" direction="oc"/>
<pin name="A2" direction="oc"/>
<pin name="A3" direction="oc"/>
<pin name="A4" direction="oc"/>
<pin name="A5" direction="oc"/>
<pin name="A6" direction="oc"/>
<pin name="A7" direction="oc"/>
<pin name="A8" direction="oc"/>
<pin name="B8" direction="oc"/>
<pin name="B7" direction="oc"/>
<pin name="B6" direction="oc"/>
<pin name="B5" direction="oc"/>
<pin name="B4" direction="oc"/>
<pin name="B3" direction="oc"/>
<pin name="B2" direction="oc"/>
<pin name="B1" direction="oc"/>
<pin name="GBA" direction="in" function="dot"/>
</symbol>
<symbol name="74651">
<pin name="CAB" direction="in" function="clk"/>
<pin name="SAB" direction="in"/>
<pin name="GAB" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="GBA" direction="in" function="dot"/>
<pin name="SBA" direction="in"/>
<pin name="CBA" direction="in" function="clk"/>
</symbol>
<symbol name="74668">
<pin name="U/!D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="ENP" direction="in" function="dot"/>
<pin name="LD" direction="in" function="dot"/>
<pin name="ENT" direction="in" function="dot"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="RCO" direction="out" function="dot"/>
</symbol>
<symbol name="74670">
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="RB" direction="in"/>
<pin name="RA" direction="in"/>
<pin name="Q4" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q1" direction="hiz"/>
<pin name="GR" direction="in" function="dot"/>
<pin name="GW" direction="in" function="dot"/>
<pin name="WB" direction="in"/>
<pin name="WA" direction="in"/>
<pin name="D1" direction="in"/>
</symbol>
<symbol name="74671">
<pin name="SRR" direction="in"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="SRL" direction="in"/>
<pin name="SCL" direction="in" function="dot"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="R/!S" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="QD" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QB" direction="hiz"/>
<pin name="QA" direction="hiz"/>
<pin name="CASC" direction="out" function="dot"/>
</symbol>
<symbol name="74673">
<pin name="CS" direction="in" function="dot"/>
<pin name="SHCLK" direction="in" function="clk"/>
<pin name="R/!W" direction="in"/>
<pin name="STRCLR" direction="in" function="dot"/>
<pin name="M/SCLK" direction="in" function="clk"/>
<pin name="SER/Q15"/>
<pin name="Y0" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
<pin name="Y9" direction="out"/>
<pin name="Y10" direction="out"/>
<pin name="Y11" direction="out"/>
<pin name="Y12" direction="out"/>
<pin name="Y13" direction="out"/>
<pin name="Y14" direction="out"/>
<pin name="Y15" direction="out"/>
</symbol>
<symbol name="74674">
<pin name="CS" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="R/!W" direction="in"/>
<pin name="MOD" direction="in"/>
<pin name="SER/Q15"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="P8" direction="in"/>
<pin name="P9" direction="in"/>
<pin name="P10" direction="in"/>
<pin name="P11" direction="in"/>
<pin name="P12" direction="in"/>
<pin name="P13" direction="in"/>
<pin name="P14" direction="in"/>
<pin name="P15" direction="in"/>
</symbol>
<symbol name="74678">
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Y" direction="out" function="dot"/>
<pin name="G" direction="in"/>
</symbol>
<symbol name="74679">
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Y" direction="out" function="dot"/>
<pin name="G" direction="in" function="dot"/>
</symbol>
<symbol name="74680">
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Y" direction="out" function="dot"/>
<pin name="G" direction="in"/>
</symbol>
<symbol name="74681">
<pin name="CLK" direction="in" function="clk"/>
<pin name="RS2" direction="in"/>
<pin name="RS1" direction="in"/>
<pin name="RS0" direction="in"/>
<pin name="LI/RO"/>
<pin name="CN" direction="in"/>
<pin name="G" direction="out" function="dot"/>
<pin name="CN+4" direction="out"/>
<pin name="P" direction="out" function="dot"/>
<pin name="I/O3"/>
<pin name="I/O2"/>
<pin name="I/O1"/>
<pin name="I/O0"/>
<pin name="MOD" direction="in"/>
<pin name="AS2" direction="in"/>
<pin name="AS1" direction="in"/>
<pin name="AS0" direction="in"/>
<pin name="RI/LO"/>
</symbol>
<symbol name="74682">
<pin name="P&gt;Q" direction="out" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="out" function="dot"/>
</symbol>
<symbol name="74683">
<pin name="P&gt;Q" direction="oc" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="oc" function="dot"/>
</symbol>
<symbol name="74686">
<pin name="P&gt;Q" direction="out" function="dot"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="out" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74687">
<pin name="P&gt;Q" direction="oc" function="dot"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="oc" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74688">
<pin name="G" direction="in" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="out" function="dot"/>
</symbol>
<symbol name="74689">
<pin name="G" direction="in" function="dot"/>
<pin name="P0" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="P=Q" direction="oc" function="dot"/>
</symbol>
<symbol name="74690">
<pin name="CCL" direction="in" function="dot"/>
<pin name="CCK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="RCL" direction="in" function="dot"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="R/!C" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="LD" direction="in" function="dot"/>
<pin name="ENT" direction="in"/>
<pin name="QD" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QB" direction="hiz"/>
<pin name="QA" direction="hiz"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="74696">
<pin name="U/!D" direction="in"/>
<pin name="CCK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="ENP" direction="in" function="dot"/>
<pin name="CCL" direction="in" function="dot"/>
<pin name="RCK" direction="in" function="clk"/>
<pin name="R/!C" direction="in"/>
<pin name="G" direction="in" function="dot"/>
<pin name="LD" direction="in" function="dot"/>
<pin name="ENT" direction="in" function="dot"/>
<pin name="QD" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QB" direction="hiz"/>
<pin name="QA" direction="hiz"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="74746">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="Y8" direction="out" function="dot"/>
<pin name="Y7" direction="out" function="dot"/>
<pin name="Y6" direction="out" function="dot"/>
<pin name="Y5" direction="out" function="dot"/>
<pin name="Y4" direction="out" function="dot"/>
<pin name="Y3" direction="out" function="dot"/>
<pin name="Y2" direction="out" function="dot"/>
<pin name="Y1" direction="out" function="dot"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74747">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="Y8" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="G2" direction="in" function="dot"/>
</symbol>
<symbol name="74756">
<pin name="G" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="oc" function="dot"/>
<pin name="Y3" direction="oc" function="dot"/>
<pin name="Y2" direction="oc" function="dot"/>
<pin name="Y1" direction="oc" function="dot"/>
</symbol>
<symbol name="74762">
<pin name="G" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="oc" function="dot"/>
<pin name="Y3" direction="oc" function="dot"/>
<pin name="Y2" direction="oc" function="dot"/>
<pin name="Y1" direction="oc" function="dot"/>
</symbol>
<symbol name="74763">
<pin name="G1" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="oc" function="dot"/>
<pin name="Y3" direction="oc" function="dot"/>
<pin name="Y2" direction="oc" function="dot"/>
<pin name="Y1" direction="oc" function="dot"/>
</symbol>
<symbol name="74804">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="74805">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="74808">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="74811">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="74832">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="74850">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="GY" direction="in" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="GW" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="W" direction="hiz" function="dot"/>
<pin name="S3" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="Y" direction="hiz"/>
<pin name="D15" direction="in"/>
<pin name="D14" direction="in"/>
<pin name="D13" direction="in"/>
<pin name="D12" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D8" direction="in"/>
</symbol>
<symbol name="74851">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="GY" direction="in" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="GW" direction="in"/>
<pin name="SC" direction="in" function="dot"/>
<pin name="W" direction="hiz" function="dot"/>
<pin name="S3" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="Y" direction="hiz"/>
<pin name="D15" direction="in"/>
<pin name="D14" direction="in"/>
<pin name="D13" direction="in"/>
<pin name="D12" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D8" direction="in"/>
</symbol>
<symbol name="74852">
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="Q8" direction="hiz"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="SRI" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="74856">
<pin name="OEB" direction="in" function="dot"/>
<pin name="OEA" direction="in" function="dot"/>
<pin name="MOD" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="Q8" direction="hiz"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="SRI" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="74857">
<pin name="S0" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2Y" direction="hiz"/>
<pin name="3A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3Y" direction="hiz"/>
<pin name="O=0" direction="hiz"/>
<pin name="CMP" direction="in"/>
<pin name="4Y" direction="hiz"/>
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="5Y" direction="hiz"/>
<pin name="5B" direction="in"/>
<pin name="5A" direction="in"/>
<pin name="6Y" direction="hiz"/>
<pin name="6B" direction="in"/>
<pin name="6A" direction="in"/>
<pin name="S1" direction="in"/>
</symbol>
<symbol name="74866">
<pin name="QLE" direction="in"/>
<pin name="L/!A" direction="in"/>
<pin name="P&lt;Q_I" direction="in"/>
<pin name="P&gt;Q_I" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P=Q_O" direction="oc"/>
<pin name="OLE" direction="in"/>
<pin name="P&gt;Q_O" direction="oc"/>
<pin name="P&lt;Q_0" direction="oc"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="PLE" direction="in"/>
<pin name="CLRQ" direction="in" function="dot"/>
</symbol>
<symbol name="74867">
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="ENT" direction="in" function="dot"/>
<pin name="RCO" direction="out" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="QH" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="ENP" direction="in" function="dot"/>
</symbol>
<symbol name="74873">
<pin name="CLR" direction="in" function="dot"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="Q4" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q1" direction="hiz"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="74874">
<pin name="CLR" direction="in" function="dot"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="Q4" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q1" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="74876">
<pin name="PRE" direction="in" function="dot"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="Q4" direction="hiz"/>
<pin name="Q3" direction="hiz"/>
<pin name="Q2" direction="hiz"/>
<pin name="Q1" direction="hiz"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="74877">
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="Q8" direction="hiz"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="SRI" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="74879">
<pin name="CLR" direction="in" function="dot"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="Q4" direction="hiz" function="dot"/>
<pin name="Q3" direction="hiz" function="dot"/>
<pin name="Q2" direction="hiz" function="dot"/>
<pin name="Q1" direction="hiz" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
</symbol>
<symbol name="74880">
<pin name="PRE" direction="in" function="dot"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="Q4" direction="hiz" function="dot"/>
<pin name="Q3" direction="hiz" function="dot"/>
<pin name="Q2" direction="hiz" function="dot"/>
<pin name="Q1" direction="hiz" function="dot"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="74882">
<pin name="CN" direction="in"/>
<pin name="G0" direction="in" function="dot"/>
<pin name="P0" direction="in" function="dot"/>
<pin name="G1" direction="in" function="dot"/>
<pin name="P1" direction="in" function="dot"/>
<pin name="CN+8" direction="out"/>
<pin name="G2" direction="in" function="dot"/>
<pin name="P2" direction="in" function="dot"/>
<pin name="G3" direction="in" function="dot"/>
<pin name="P3" direction="in" function="dot"/>
<pin name="CN+16" direction="out"/>
<pin name="G4" direction="in" function="dot"/>
<pin name="P4" direction="in" function="dot"/>
<pin name="G5" direction="in" function="dot"/>
<pin name="P5" direction="in" function="dot"/>
<pin name="CN+24" direction="out"/>
<pin name="G6" direction="in" function="dot"/>
<pin name="P6" direction="in" function="dot"/>
<pin name="G7" direction="in" function="dot"/>
<pin name="P7" direction="in" function="dot"/>
<pin name="CN+32" direction="out"/>
</symbol>
<symbol name="74885">
<pin name="L/!A" direction="in"/>
<pin name="P&lt;Q_I" direction="in"/>
<pin name="P&gt;Q_I" direction="in"/>
<pin name="Q7" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P&gt;Q_O" direction="out"/>
<pin name="P&lt;Q_0" direction="out"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="PLE" direction="in"/>
</symbol>
<symbol name="74757">
<pin name="G" direction="in" function="dot"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="oc"/>
<pin name="Y3" direction="oc"/>
<pin name="Y2" direction="oc"/>
<pin name="Y1" direction="oc"/>
</symbol>
<symbol name="74533">
<pin name="OC" direction="in" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="C" direction="in"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="8Q" direction="hiz" function="dot"/>
</symbol>
<symbol name="74534">
<pin name="OC" direction="in" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="8Q" direction="hiz" function="dot"/>
</symbol>
<symbol name="74563">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="8Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
</symbol>
<symbol name="74564">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="8Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
</symbol>
<symbol name="74573">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74574">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74575">
<pin name="CLR" direction="in" function="dot"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74576">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="8Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
</symbol>
<symbol name="74577">
<pin name="CLR" direction="in" function="dot"/>
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="8Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
</symbol>
<symbol name="74580">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="8Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
</symbol>
<symbol name="74821">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="9D" direction="in"/>
<pin name="10D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="10Q" direction="hiz"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74822">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in" function="dot"/>
<pin name="2D" direction="in" function="dot"/>
<pin name="3D" direction="in" function="dot"/>
<pin name="4D" direction="in" function="dot"/>
<pin name="5D" direction="in" function="dot"/>
<pin name="6D" direction="in" function="dot"/>
<pin name="7D" direction="in" function="dot"/>
<pin name="8D" direction="in" function="dot"/>
<pin name="9D" direction="in" function="dot"/>
<pin name="10D" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="10Q" direction="hiz"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74823">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="9D" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLKEN" direction="in" function="dot"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74824">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in" function="dot"/>
<pin name="2D" direction="in" function="dot"/>
<pin name="3D" direction="in" function="dot"/>
<pin name="4D" direction="in" function="dot"/>
<pin name="5D" direction="in" function="dot"/>
<pin name="6D" direction="in" function="dot"/>
<pin name="7D" direction="in" function="dot"/>
<pin name="8D" direction="in" function="dot"/>
<pin name="9D" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLKEN" direction="in" function="dot"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74825">
<pin name="OC1" direction="in" function="dot"/>
<pin name="OC2" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLKEN" direction="in" function="dot"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="OC3" direction="in" function="dot"/>
</symbol>
<symbol name="74826">
<pin name="OC1" direction="in" function="dot"/>
<pin name="OC2" direction="in" function="dot"/>
<pin name="1D" direction="in" function="dot"/>
<pin name="2D" direction="in" function="dot"/>
<pin name="3D" direction="in" function="dot"/>
<pin name="4D" direction="in" function="dot"/>
<pin name="5D" direction="in" function="dot"/>
<pin name="6D" direction="in" function="dot"/>
<pin name="7D" direction="in" function="dot"/>
<pin name="8D" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLKEN" direction="in" function="dot"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="OC3" direction="in" function="dot"/>
</symbol>
<symbol name="74841">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="9D" direction="in"/>
<pin name="10D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="10Q" direction="hiz"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74842">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in" function="dot"/>
<pin name="2D" direction="in" function="dot"/>
<pin name="3D" direction="in" function="dot"/>
<pin name="4D" direction="in" function="dot"/>
<pin name="5D" direction="in" function="dot"/>
<pin name="6D" direction="in" function="dot"/>
<pin name="7D" direction="in" function="dot"/>
<pin name="8D" direction="in" function="dot"/>
<pin name="9D" direction="in" function="dot"/>
<pin name="10D" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="10Q" direction="hiz"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74843">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="9D" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74844">
<pin name="OC" direction="in" function="dot"/>
<pin name="1D" direction="in" function="dot"/>
<pin name="2D" direction="in" function="dot"/>
<pin name="3D" direction="in" function="dot"/>
<pin name="4D" direction="in" function="dot"/>
<pin name="5D" direction="in" function="dot"/>
<pin name="6D" direction="in" function="dot"/>
<pin name="7D" direction="in" function="dot"/>
<pin name="8D" direction="in" function="dot"/>
<pin name="9D" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74845">
<pin name="OC1" direction="in" function="dot"/>
<pin name="OC2" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="OC3" direction="in" function="dot"/>
</symbol>
<symbol name="74846">
<pin name="OC1" direction="in" function="dot"/>
<pin name="OC2" direction="in" function="dot"/>
<pin name="1D" direction="in" function="dot"/>
<pin name="2D" direction="in" function="dot"/>
<pin name="3D" direction="in" function="dot"/>
<pin name="4D" direction="in" function="dot"/>
<pin name="5D" direction="in" function="dot"/>
<pin name="6D" direction="in" function="dot"/>
<pin name="7D" direction="in" function="dot"/>
<pin name="8D" direction="in" function="dot"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="OC3" direction="in" function="dot"/>
</symbol>
<symbol name="74990">
<pin name="OERB" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="8Q" direction="out"/>
<pin name="7Q" direction="out"/>
<pin name="6Q" direction="out"/>
<pin name="5Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="1Q" direction="out"/>
</symbol>
<symbol name="74991">
<pin name="OERB" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="8Q" direction="out" function="dot"/>
<pin name="7Q" direction="out" function="dot"/>
<pin name="6Q" direction="out" function="dot"/>
<pin name="5Q" direction="out" function="dot"/>
<pin name="4Q" direction="out" function="dot"/>
<pin name="3Q" direction="out" function="dot"/>
<pin name="2Q" direction="out" function="dot"/>
<pin name="1Q" direction="out" function="dot"/>
</symbol>
<symbol name="74992">
<pin name="OERB" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="9D" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="OEQ" direction="in" function="dot"/>
<pin name="9Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="74993">
<pin name="OERB" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="9D" direction="in"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="OEQ" direction="in" function="dot"/>
<pin name="9Q" direction="hiz" function="dot"/>
<pin name="8Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
</symbol>
<symbol name="74994">
<pin name="OERB" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="9D" direction="in"/>
<pin name="10D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="10Q" direction="out"/>
<pin name="9Q" direction="out"/>
<pin name="8Q" direction="out"/>
<pin name="7Q" direction="out"/>
<pin name="6Q" direction="out"/>
<pin name="5Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="1Q" direction="out"/>
</symbol>
<symbol name="74995">
<pin name="OERB" direction="in" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="6D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="9D" direction="in"/>
<pin name="10D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="10Q" direction="out" function="dot"/>
<pin name="9Q" direction="out" function="dot"/>
<pin name="8Q" direction="out" function="dot"/>
<pin name="7Q" direction="out" function="dot"/>
<pin name="6Q" direction="out" function="dot"/>
<pin name="5Q" direction="out" function="dot"/>
<pin name="4Q" direction="out" function="dot"/>
<pin name="3Q" direction="out" function="dot"/>
<pin name="2Q" direction="out" function="dot"/>
<pin name="1Q" direction="out" function="dot"/>
</symbol>
<symbol name="74543">
<pin name="GBA" direction="in" function="dot"/>
<pin name="CEBA" direction="in" function="dot"/>
<pin name="LEBA" direction="in" function="dot"/>
<pin name="GAB" direction="in" function="dot"/>
<pin name="CEAB" direction="in" function="dot"/>
<pin name="LEAB" direction="in" function="dot"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B1" direction="hiz"/>
<pin name="B2" direction="hiz"/>
<pin name="B3" direction="hiz"/>
<pin name="B4" direction="hiz"/>
<pin name="B5" direction="hiz"/>
<pin name="B6" direction="hiz"/>
<pin name="B7" direction="hiz"/>
<pin name="B8" direction="hiz"/>
</symbol>
<symbol name="74657">
<pin name="!G" direction="in"/>
<pin name="T/R" direction="in" function="dot"/>
<pin name="ODD/!EVN" direction="in"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="PARITY"/>
<pin name="!ERR" direction="hiz"/>
</symbol>
<symbol name="PWR2GND">
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="74616">
<pin name="LEDBO" direction="hiz" function="dot"/>
<pin name="MERR" direction="out" function="dot"/>
<pin name="ERR" direction="out" function="dot"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="OEB0" direction="hiz" function="dot"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="CB5"/>
<pin name="CB4"/>
<pin name="OECB" direction="hiz" function="dot"/>
<pin name="CB3"/>
<pin name="CB2"/>
<pin name="CB1"/>
<pin name="CB0"/>
<pin name="DB8"/>
<pin name="DB9"/>
<pin name="DB10"/>
<pin name="DB11"/>
<pin name="DB12"/>
<pin name="DB13"/>
<pin name="OEB1" direction="hiz" function="dot"/>
<pin name="DB14"/>
<pin name="DB15"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
</symbol>
<symbol name="74617">
<pin name="LEDBO" direction="oc" function="dot"/>
<pin name="MERR" direction="out" function="dot"/>
<pin name="ERR" direction="out" function="dot"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="OEB0" direction="oc" function="dot"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="CB5"/>
<pin name="CB4"/>
<pin name="OECB" direction="oc" function="dot"/>
<pin name="CB3"/>
<pin name="CB2"/>
<pin name="CB1"/>
<pin name="CB0"/>
<pin name="DB8"/>
<pin name="DB9"/>
<pin name="DB10"/>
<pin name="DB11"/>
<pin name="DB12"/>
<pin name="DB13"/>
<pin name="OEB1" direction="oc" function="dot"/>
<pin name="DB14"/>
<pin name="DB15"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
</symbol>
<symbol name="74634">
<pin name="MERR" direction="out" function="dot"/>
<pin name="ERR" direction="out" function="dot"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="OEDB" direction="hiz" function="dot"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DB8"/>
<pin name="DB9"/>
<pin name="DB10"/>
<pin name="DB11"/>
<pin name="DB12"/>
<pin name="DB13"/>
<pin name="DB14"/>
<pin name="DB15"/>
<pin name="CB6"/>
<pin name="CB5"/>
<pin name="CB4"/>
<pin name="OECB" direction="hiz" function="dot"/>
<pin name="CB3"/>
<pin name="CB2"/>
<pin name="CB1"/>
<pin name="CB0"/>
<pin name="DB16"/>
<pin name="DB17"/>
<pin name="DB18"/>
<pin name="DB19"/>
<pin name="DB20"/>
<pin name="DB21"/>
<pin name="DB22"/>
<pin name="DB23"/>
<pin name="DB24"/>
<pin name="DB25"/>
<pin name="DB26"/>
<pin name="DB27"/>
<pin name="DB28"/>
<pin name="DB29"/>
<pin name="DB30"/>
<pin name="DB31"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
</symbol>
<symbol name="74635">
<pin name="MERR" direction="out" function="dot"/>
<pin name="ERR" direction="out" function="dot"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="OEDB" direction="oc" function="dot"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DB8"/>
<pin name="DB9"/>
<pin name="DB10"/>
<pin name="DB11"/>
<pin name="DB12"/>
<pin name="DB13"/>
<pin name="DB14"/>
<pin name="DB15"/>
<pin name="CB6"/>
<pin name="CB5"/>
<pin name="CB4"/>
<pin name="OECB" direction="oc" function="dot"/>
<pin name="CB3"/>
<pin name="CB2"/>
<pin name="CB1"/>
<pin name="CB0"/>
<pin name="DB16"/>
<pin name="DB17"/>
<pin name="DB18"/>
<pin name="DB19"/>
<pin name="DB20"/>
<pin name="DB21"/>
<pin name="DB22"/>
<pin name="DB23"/>
<pin name="DB24"/>
<pin name="DB25"/>
<pin name="DB26"/>
<pin name="DB27"/>
<pin name="DB28"/>
<pin name="DB29"/>
<pin name="DB30"/>
<pin name="DB31"/>
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
</symbol>
<symbol name="74666">
<pin name="OERB" direction="in" function="dot"/>
<pin name="OE1" direction="in" function="dot"/>
<pin name="1D"/>
<pin name="2D"/>
<pin name="3D"/>
<pin name="4D"/>
<pin name="5D"/>
<pin name="6D"/>
<pin name="7D"/>
<pin name="8D"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="OE2" direction="in" function="dot"/>
</symbol>
<symbol name="74667">
<pin name="OERB" direction="in" function="dot"/>
<pin name="OE1" direction="in" function="dot"/>
<pin name="1D"/>
<pin name="2D"/>
<pin name="3D"/>
<pin name="4D"/>
<pin name="5D"/>
<pin name="6D"/>
<pin name="7D"/>
<pin name="8D"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="C" direction="in"/>
<pin name="PRE" direction="in" function="dot"/>
<pin name="8Q" direction="hiz" function="dot"/>
<pin name="7Q" direction="hiz" function="dot"/>
<pin name="6Q" direction="hiz" function="dot"/>
<pin name="5Q" direction="hiz" function="dot"/>
<pin name="4Q" direction="hiz" function="dot"/>
<pin name="3Q" direction="hiz" function="dot"/>
<pin name="2Q" direction="hiz" function="dot"/>
<pin name="1Q" direction="hiz" function="dot"/>
<pin name="OE2" direction="in" function="dot"/>
</symbol>
<symbol name="74870">
<pin name="S0" direction="in"/>
<pin name="1A0" direction="in"/>
<pin name="1A1" direction="in"/>
<pin name="1A2" direction="in"/>
<pin name="1A3" direction="in"/>
<pin name="1W" direction="in" function="dot"/>
<pin name="S2" direction="in"/>
<pin name="DQA1"/>
<pin name="DQA2"/>
<pin name="DQA3"/>
<pin name="DQA4"/>
<pin name="DQB1"/>
<pin name="DQB2"/>
<pin name="DQB3"/>
<pin name="DQB4"/>
<pin name="S3" direction="in"/>
<pin name="2W" direction="in" function="dot"/>
<pin name="2A0" direction="in"/>
<pin name="2A1" direction="in"/>
<pin name="2A2" direction="in"/>
<pin name="2A3" direction="in"/>
<pin name="S1" direction="in"/>
</symbol>
<symbol name="74871">
<pin name="DA1" direction="in"/>
<pin name="DA2" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="1A0" direction="in"/>
<pin name="1A1" direction="in"/>
<pin name="1A2" direction="in"/>
<pin name="1A3" direction="in"/>
<pin name="1W" direction="in" function="dot"/>
<pin name="S2" direction="in"/>
<pin name="QA1" direction="out"/>
<pin name="QA2" direction="out"/>
<pin name="QA3" direction="out"/>
<pin name="QA4" direction="out"/>
<pin name="DQB1"/>
<pin name="DQB2"/>
<pin name="DQB3"/>
<pin name="DQB4"/>
<pin name="S3" direction="in"/>
<pin name="2W" direction="in" function="dot"/>
<pin name="2A0" direction="in"/>
<pin name="2A1" direction="in"/>
<pin name="2A2" direction="in"/>
<pin name="2A3" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="DA3" direction="in"/>
<pin name="DA4" direction="in"/>
</symbol>
<symbol name="74963">
<pin name="OE" direction="in" function="dot"/>
<pin name="SERIN" direction="in"/>
<pin name="GIN" direction="in" function="dot"/>
<pin name="G2-1" direction="in" function="dot"/>
<pin name="SCLR" direction="in"/>
<pin name="G1-2" direction="in" function="dot"/>
<pin name="GSH" direction="in" function="dot"/>
<pin name="SEROUT" direction="out"/>
<pin name="CLK2" direction="in" function="clk"/>
<pin name="CLK1" direction="in" function="clk"/>
<pin name="H/QH"/>
<pin name="G/QG"/>
<pin name="F/QF"/>
<pin name="E/QE"/>
<pin name="D/QD"/>
<pin name="C/QC"/>
<pin name="B/QB"/>
<pin name="A/QA"/>
</symbol>
<symbol name="74964">
<pin name="OE" direction="in" function="dot"/>
<pin name="SERIN" direction="in"/>
<pin name="GIN" direction="in" function="dot"/>
<pin name="G2-1" direction="in" function="dot"/>
<pin name="SCLR" direction="in"/>
<pin name="G1-2" direction="in" function="dot"/>
<pin name="GSH" direction="in" function="dot"/>
<pin name="SEROUT" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="ACLR" direction="in"/>
<pin name="H/QH"/>
<pin name="G/QG"/>
<pin name="F/QF"/>
<pin name="E/QE"/>
<pin name="D/QD"/>
<pin name="C/QC"/>
<pin name="B/QB"/>
<pin name="A/QA"/>
</symbol>
<symbol name="74996">
<pin name="1D"/>
<pin name="2D"/>
<pin name="3D"/>
<pin name="4D"/>
<pin name="5D"/>
<pin name="6D"/>
<pin name="7D"/>
<pin name="8D"/>
<pin name="EN" direction="in" function="dot"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="CLR" direction="in" function="dot"/>
<pin name="T/!C" direction="in" function="dot"/>
<pin name="G" direction="in" function="dot"/>
<pin name="8Q" direction="hiz"/>
<pin name="7Q" direction="hiz"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
</symbol>
<symbol name="2PWR4GND">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="74805EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="74811EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="74832EU">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="74241A">
<pin name="G" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="74305">
<pin name="PRE" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="RST" direction="in" function="dot"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out" function="dot"/>
<pin name="Q6" direction="out" function="dot"/>
<pin name="Q7" direction="out" function="dot"/>
<pin name="Q8" direction="out" function="dot"/>
</symbol>
<symbol name="7414">
<pin name="I" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="74S51">
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2C" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Y" direction="out" function="dot"/>
<pin name="1Y" direction="out" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1C" direction="in"/>
</symbol>
<symbol name="74LS51">
<pin name="1A" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2C" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="2Y" direction="out" function="dot"/>
<pin name="1Y" direction="out" function="dot"/>
<pin name="1D" direction="in"/>
<pin name="1E" direction="in"/>
<pin name="1F" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1C" direction="in"/>
</symbol>
<symbol name="74624">
<pin name="RANGE" direction="in"/>
<pin name="XTC@1" direction="pas"/>
<pin name="XTC@2" direction="pas"/>
<pin name="EN" direction="in" function="dot"/>
<pin name="FCTR" direction="in"/>
<pin name="!Q" direction="out"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="74132">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="74HC73">
<pin name="CP" direction="in" function="dot"/>
<pin name="R" direction="in" function="dot"/>
<pin name="K" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="J" direction="in"/>
</symbol>
<symbol name="7447">
<pin name="IB" direction="in"/>
<pin name="IC" direction="in"/>
<pin name="LT" direction="in" function="dot"/>
<pin name="BI/RBO" direction="in" function="dot"/>
<pin name="RBI" direction="in" function="dot"/>
<pin name="ID" direction="in"/>
<pin name="IA" direction="in"/>
<pin name="E" direction="out"/>
<pin name="D" direction="out"/>
<pin name="C" direction="out"/>
<pin name="B" direction="out"/>
<pin name="A" direction="out"/>
<pin name="G" direction="out"/>
<pin name="F" direction="out"/>
</symbol>
<symbol name="74190-1">
<pin name="B" direction="in"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CTE" direction="in" function="dot"/>
<pin name="D/!U" direction="in"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="LD" direction="in" function="dot"/>
<pin name="MX/MN" direction="out"/>
<pin name="RCO" direction="out" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="PWRN-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74922">
<pin name="Y1" direction="in"/>
<pin name="Y2" direction="in"/>
<pin name="Y3" direction="in"/>
<pin name="Y4" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="KBM" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="X3" direction="in"/>
<pin name="X4" direction="in"/>
<pin name="DATA_AV" direction="out"/>
<pin name="!OE" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="PWRN-2">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74923">
<pin name="Y1" direction="in"/>
<pin name="Y2" direction="in"/>
<pin name="Y3" direction="in"/>
<pin name="Y4" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="KBM" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="X3" direction="in"/>
<pin name="X4" direction="in"/>
<pin name="DATA_AV" direction="out"/>
<pin name="!OE" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="Y5" direction="in"/>
<pin name="OUTE" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74*04" prefix="IC">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7404"/>
<gate name="B" symbol="7404"/>
<gate name="C" symbol="7404"/>
<gate name="D" symbol="7404"/>
<gate name="E" symbol="7404"/>
<gate name="F" symbol="7404"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I" pad="4"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="12"/>
<connect gate="E" pin="I" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I" pad="19"/>
<connect gate="F" pin="O" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*05" prefix="IC">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="7405"/>
<gate name="B" symbol="7405"/>
<gate name="C" symbol="7405"/>
<gate name="D" symbol="7405"/>
<gate name="E" symbol="7405"/>
<gate name="F" symbol="7405"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I" pad="4"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="12"/>
<connect gate="E" pin="I" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I" pad="19"/>
<connect gate="F" pin="O" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*07" prefix="IC">
<description>Hex &lt;b&gt;BUFFER&lt;/b&gt;, open collector high-voltage output</description>
<gates>
<gate name="A" symbol="7407"/>
<gate name="B" symbol="7407"/>
<gate name="C" symbol="7407"/>
<gate name="D" symbol="7407"/>
<gate name="E" symbol="7407"/>
<gate name="F" symbol="7407"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*42" prefix="IC">
<description>4-line to 10-line &lt;b&gt;DECODER&lt;/b&gt; (1-of-10)</description>
<gates>
<gate name="A" symbol="7442"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="O0" pad="1"/>
<connect gate="A" pin="O1" pad="2"/>
<connect gate="A" pin="O2" pad="3"/>
<connect gate="A" pin="O3" pad="4"/>
<connect gate="A" pin="O4" pad="5"/>
<connect gate="A" pin="O5" pad="6"/>
<connect gate="A" pin="O6" pad="7"/>
<connect gate="A" pin="O7" pad="9"/>
<connect gate="A" pin="O8" pad="10"/>
<connect gate="A" pin="O9" pad="11"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="O0" pad="1"/>
<connect gate="A" pin="O1" pad="2"/>
<connect gate="A" pin="O2" pad="3"/>
<connect gate="A" pin="O3" pad="4"/>
<connect gate="A" pin="O4" pad="5"/>
<connect gate="A" pin="O5" pad="6"/>
<connect gate="A" pin="O6" pad="7"/>
<connect gate="A" pin="O7" pad="9"/>
<connect gate="A" pin="O8" pad="10"/>
<connect gate="A" pin="O9" pad="11"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="19"/>
<connect gate="A" pin="B" pad="18"/>
<connect gate="A" pin="C" pad="17"/>
<connect gate="A" pin="D" pad="15"/>
<connect gate="A" pin="O0" pad="2"/>
<connect gate="A" pin="O1" pad="3"/>
<connect gate="A" pin="O2" pad="4"/>
<connect gate="A" pin="O3" pad="5"/>
<connect gate="A" pin="O4" pad="7"/>
<connect gate="A" pin="O5" pad="8"/>
<connect gate="A" pin="O6" pad="9"/>
<connect gate="A" pin="O7" pad="12"/>
<connect gate="A" pin="O8" pad="13"/>
<connect gate="A" pin="O9" pad="14"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*45" prefix="IC">
<description>BCD to decimal &lt;b&gt;DECODER/DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7445"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="O0" pad="1"/>
<connect gate="A" pin="O1" pad="2"/>
<connect gate="A" pin="O2" pad="3"/>
<connect gate="A" pin="O3" pad="4"/>
<connect gate="A" pin="O4" pad="5"/>
<connect gate="A" pin="O5" pad="6"/>
<connect gate="A" pin="O6" pad="7"/>
<connect gate="A" pin="O7" pad="9"/>
<connect gate="A" pin="O8" pad="10"/>
<connect gate="A" pin="O9" pad="11"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="O0" pad="1"/>
<connect gate="A" pin="O1" pad="2"/>
<connect gate="A" pin="O2" pad="3"/>
<connect gate="A" pin="O3" pad="4"/>
<connect gate="A" pin="O4" pad="5"/>
<connect gate="A" pin="O5" pad="6"/>
<connect gate="A" pin="O6" pad="7"/>
<connect gate="A" pin="O7" pad="9"/>
<connect gate="A" pin="O8" pad="10"/>
<connect gate="A" pin="O9" pad="11"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*46" prefix="IC">
<description>BCD to seven segment &lt;b&gt;DECODER/DRIVER&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="7446"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="BI/RBO" pad="4"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="D" pad="10"/>
<connect gate="A" pin="E" pad="9"/>
<connect gate="A" pin="F" pad="15"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="IA" pad="7"/>
<connect gate="A" pin="IB" pad="1"/>
<connect gate="A" pin="IC" pad="2"/>
<connect gate="A" pin="ID" pad="6"/>
<connect gate="A" pin="LT" pad="3"/>
<connect gate="A" pin="RBI" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*48" prefix="IC">
<description>BCD to seven segment &lt;b&gt;DECODER/DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7448"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="BI/RBO" pad="4"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="D" pad="10"/>
<connect gate="A" pin="E" pad="9"/>
<connect gate="A" pin="F" pad="15"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="IA" pad="7"/>
<connect gate="A" pin="IB" pad="1"/>
<connect gate="A" pin="IC" pad="2"/>
<connect gate="A" pin="ID" pad="6"/>
<connect gate="A" pin="LT" pad="3"/>
<connect gate="A" pin="RBI" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*49" prefix="IC">
<description>BCD to seven segment &lt;b&gt;DECODER/DRIVER&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="7449"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="BI" pad="3"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="D" pad="8"/>
<connect gate="A" pin="E" pad="6"/>
<connect gate="A" pin="F" pad="13"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="IA" pad="5"/>
<connect gate="A" pin="IB" pad="1"/>
<connect gate="A" pin="IC" pad="2"/>
<connect gate="A" pin="ID" pad="4"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*50" prefix="IC">
<description>Dual 2-wide 2-input &lt;b&gt;AND OR INVERTER&lt;/b&gt; gate (one gate expandable)</description>
<gates>
<gate name="A" symbol="7450"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!1X" pad="12"/>
<connect gate="A" pin="1A" pad="1"/>
<connect gate="A" pin="1B" pad="13"/>
<connect gate="A" pin="1C" pad="9"/>
<connect gate="A" pin="1D" pad="10"/>
<connect gate="A" pin="1X" pad="11"/>
<connect gate="A" pin="1Y" pad="8"/>
<connect gate="A" pin="2A" pad="2"/>
<connect gate="A" pin="2B" pad="3"/>
<connect gate="A" pin="2C" pad="4"/>
<connect gate="A" pin="2D" pad="5"/>
<connect gate="A" pin="2Y" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*51" prefix="IC">
<description>&lt;b&gt;AND-OR-INVERT&lt;/b&gt; gates/for S-type see &lt;a href=DEVICE:74S51&gt;74S51&lt;/a&gt;</description>
<gates>
<gate name="A" symbol="74LS51"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="1A" pad="1"/>
<connect gate="A" pin="1B" pad="12"/>
<connect gate="A" pin="1C" pad="13"/>
<connect gate="A" pin="1D" pad="9"/>
<connect gate="A" pin="1E" pad="10"/>
<connect gate="A" pin="1F" pad="11"/>
<connect gate="A" pin="1Y" pad="8"/>
<connect gate="A" pin="2A" pad="2"/>
<connect gate="A" pin="2B" pad="3"/>
<connect gate="A" pin="2C" pad="4"/>
<connect gate="A" pin="2D" pad="5"/>
<connect gate="A" pin="2Y" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="1A" pad="1"/>
<connect gate="A" pin="1B" pad="12"/>
<connect gate="A" pin="1C" pad="13"/>
<connect gate="A" pin="1D" pad="9"/>
<connect gate="A" pin="1E" pad="10"/>
<connect gate="A" pin="1F" pad="11"/>
<connect gate="A" pin="1Y" pad="8"/>
<connect gate="A" pin="2A" pad="2"/>
<connect gate="A" pin="2B" pad="3"/>
<connect gate="A" pin="2C" pad="4"/>
<connect gate="A" pin="2D" pad="5"/>
<connect gate="A" pin="2Y" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="PLCC20">
<connects>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="18"/>
<connect gate="A" pin="1C" pad="19"/>
<connect gate="A" pin="1D" pad="13"/>
<connect gate="A" pin="1E" pad="14"/>
<connect gate="A" pin="1F" pad="16"/>
<connect gate="A" pin="1Y" pad="12"/>
<connect gate="A" pin="2A" pad="3"/>
<connect gate="A" pin="2B" pad="4"/>
<connect gate="A" pin="2C" pad="6"/>
<connect gate="A" pin="2D" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*54" prefix="IC">
<description>4-wide &lt;b&gt;AND OR INVERTER&lt;/b&gt; gates</description>
<gates>
<gate name="A" symbol="7454"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="E" pad="5"/>
<connect gate="A" pin="F" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="A" pin="H" pad="11"/>
<connect gate="A" pin="I" pad="12"/>
<connect gate="A" pin="J" pad="13"/>
<connect gate="A" pin="Y" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="E" pad="5"/>
<connect gate="A" pin="F" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="A" pin="H" pad="11"/>
<connect gate="A" pin="I" pad="12"/>
<connect gate="A" pin="J" pad="13"/>
<connect gate="A" pin="Y" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="E" pad="8"/>
<connect gate="A" pin="F" pad="13"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="H" pad="16"/>
<connect gate="A" pin="I" pad="18"/>
<connect gate="A" pin="J" pad="19"/>
<connect gate="A" pin="Y" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*55" prefix="IC">
<description>2-wide 4-input &lt;b&gt;AND OR INVERTER&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7455"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="E" pad="10"/>
<connect gate="A" pin="F" pad="11"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="H" pad="13"/>
<connect gate="A" pin="Y" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*56" prefix="IC">
<description>&lt;b&gt;FREQUENCY DIVIDER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7456"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="CKA" pad="5"/>
<connect gate="A" pin="CKB" pad="1"/>
<connect gate="A" pin="CLR" pad="6"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="7"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*63" prefix="IC">
<description>Hex current sensing &lt;b&gt;INTERFACE&lt;/b&gt; gate, totem pole</description>
<gates>
<gate name="A" symbol="7463"/>
<gate name="B" symbol="7463"/>
<gate name="C" symbol="7463"/>
<gate name="D" symbol="7463"/>
<gate name="E" symbol="7463"/>
<gate name="F" symbol="7463"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="4"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="10"/>
<connect gate="E" pin="O" pad="11"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*64" prefix="IC">
<description>4-2-3-2 input &lt;b&gt;AND OR INVERTER&lt;/b&gt; gates</description>
<gates>
<gate name="A" symbol="7464"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="11"/>
<connect gate="A" pin="I10" pad="10"/>
<connect gate="A" pin="I2" pad="12"/>
<connect gate="A" pin="I3" pad="13"/>
<connect gate="A" pin="I4" pad="2"/>
<connect gate="A" pin="I5" pad="3"/>
<connect gate="A" pin="I6" pad="4"/>
<connect gate="A" pin="I7" pad="5"/>
<connect gate="A" pin="I8" pad="6"/>
<connect gate="A" pin="I9" pad="9"/>
<connect gate="A" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="11"/>
<connect gate="A" pin="I10" pad="10"/>
<connect gate="A" pin="I2" pad="12"/>
<connect gate="A" pin="I3" pad="13"/>
<connect gate="A" pin="I4" pad="2"/>
<connect gate="A" pin="I5" pad="3"/>
<connect gate="A" pin="I6" pad="4"/>
<connect gate="A" pin="I7" pad="5"/>
<connect gate="A" pin="I8" pad="6"/>
<connect gate="A" pin="I9" pad="9"/>
<connect gate="A" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="16"/>
<connect gate="A" pin="I10" pad="14"/>
<connect gate="A" pin="I2" pad="18"/>
<connect gate="A" pin="I3" pad="19"/>
<connect gate="A" pin="I4" pad="3"/>
<connect gate="A" pin="I5" pad="4"/>
<connect gate="A" pin="I6" pad="6"/>
<connect gate="A" pin="I7" pad="8"/>
<connect gate="A" pin="I8" pad="9"/>
<connect gate="A" pin="I9" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*68" prefix="IC">
<description>Dual 4-bit decade or binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7468"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1CLKA" pad="1"/>
<connect gate="A" pin="1CLKB" pad="15"/>
<connect gate="A" pin="1CLR" pad="4"/>
<connect gate="A" pin="1QA" pad="14"/>
<connect gate="A" pin="1QB" pad="2"/>
<connect gate="A" pin="1QC" pad="13"/>
<connect gate="A" pin="1QD" pad="3"/>
<connect gate="A" pin="2CLK" pad="9"/>
<connect gate="A" pin="2CLR" pad="11"/>
<connect gate="A" pin="2QA" pad="7"/>
<connect gate="A" pin="2QB" pad="10"/>
<connect gate="A" pin="2QC" pad="5"/>
<connect gate="A" pin="2QD" pad="12"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*70" prefix="IC">
<description>AND gated J-K positive edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="A" symbol="7470"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="J" pad="5"/>
<connect gate="A" pin="J1" pad="3"/>
<connect gate="A" pin="J2" pad="4"/>
<connect gate="A" pin="K" pad="9"/>
<connect gate="A" pin="K1" pad="10"/>
<connect gate="A" pin="K2" pad="11"/>
<connect gate="A" pin="PRE" pad="13"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*72" prefix="IC">
<description>AND gated J-K master slave &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="A" symbol="7472"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="J1" pad="3"/>
<connect gate="A" pin="J2" pad="4"/>
<connect gate="A" pin="J3" pad="5"/>
<connect gate="A" pin="K1" pad="9"/>
<connect gate="A" pin="K2" pad="10"/>
<connect gate="A" pin="K3" pad="11"/>
<connect gate="A" pin="PRE" pad="13"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*73" prefix="IC">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="A" symbol="7473"/>
<gate name="B" symbol="7473"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="13"/>
<connect gate="A" pin="CL" pad="2"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="J" pad="14"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="Q" pad="12"/>
<connect gate="B" pin="!Q" pad="8"/>
<connect gate="B" pin="CL" pad="6"/>
<connect gate="B" pin="CLK" pad="5"/>
<connect gate="B" pin="J" pad="7"/>
<connect gate="B" pin="K" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="!Q" pad="13"/>
<connect gate="A" pin="CL" pad="2"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="J" pad="14"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="Q" pad="12"/>
<connect gate="B" pin="!Q" pad="8"/>
<connect gate="B" pin="CL" pad="6"/>
<connect gate="B" pin="CLK" pad="5"/>
<connect gate="B" pin="J" pad="7"/>
<connect gate="B" pin="K" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*74" prefix="IC">
<description>Dual D type positive edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="A" symbol="7474"/>
<gate name="B" symbol="7474"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="PRE" pad="4"/>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="B" pin="!Q" pad="8"/>
<connect gate="B" pin="CLK" pad="11"/>
<connect gate="B" pin="CLR" pad="13"/>
<connect gate="B" pin="D" pad="12"/>
<connect gate="B" pin="PRE" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="PRE" pad="4"/>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="B" pin="!Q" pad="8"/>
<connect gate="B" pin="CLK" pad="11"/>
<connect gate="B" pin="CLR" pad="13"/>
<connect gate="B" pin="D" pad="12"/>
<connect gate="B" pin="PRE" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!Q" pad="9"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="PRE" pad="6"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="B" pin="!Q" pad="12"/>
<connect gate="B" pin="CLK" pad="16"/>
<connect gate="B" pin="CLR" pad="19"/>
<connect gate="B" pin="D" pad="18"/>
<connect gate="B" pin="PRE" pad="14"/>
<connect gate="B" pin="Q" pad="13"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*75" prefix="IC">
<description>4-bit bistable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7475"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q1" pad="1"/>
<connect gate="A" pin="!Q2" pad="14"/>
<connect gate="A" pin="!Q3" pad="11"/>
<connect gate="A" pin="!Q4" pad="8"/>
<connect gate="A" pin="C12" pad="13"/>
<connect gate="A" pin="C34" pad="4"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="6"/>
<connect gate="A" pin="D4" pad="7"/>
<connect gate="A" pin="Q1" pad="16"/>
<connect gate="A" pin="Q2" pad="15"/>
<connect gate="A" pin="Q3" pad="10"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q1" pad="1"/>
<connect gate="A" pin="!Q2" pad="14"/>
<connect gate="A" pin="!Q3" pad="11"/>
<connect gate="A" pin="!Q4" pad="8"/>
<connect gate="A" pin="C12" pad="13"/>
<connect gate="A" pin="C34" pad="4"/>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="6"/>
<connect gate="A" pin="D4" pad="7"/>
<connect gate="A" pin="Q1" pad="16"/>
<connect gate="A" pin="Q2" pad="15"/>
<connect gate="A" pin="Q3" pad="10"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*76" prefix="IC">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="A" symbol="7476"/>
<gate name="B" symbol="7476"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q" pad="14"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="J" pad="4"/>
<connect gate="A" pin="K" pad="16"/>
<connect gate="A" pin="PRE" pad="2"/>
<connect gate="A" pin="Q" pad="15"/>
<connect gate="B" pin="!Q" pad="10"/>
<connect gate="B" pin="CLK" pad="6"/>
<connect gate="B" pin="CLR" pad="8"/>
<connect gate="B" pin="J" pad="9"/>
<connect gate="B" pin="K" pad="12"/>
<connect gate="B" pin="PRE" pad="7"/>
<connect gate="B" pin="Q" pad="11"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q" pad="14"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="J" pad="4"/>
<connect gate="A" pin="K" pad="16"/>
<connect gate="A" pin="PRE" pad="2"/>
<connect gate="A" pin="Q" pad="15"/>
<connect gate="B" pin="!Q" pad="10"/>
<connect gate="B" pin="CLK" pad="6"/>
<connect gate="B" pin="CLR" pad="8"/>
<connect gate="B" pin="J" pad="9"/>
<connect gate="B" pin="K" pad="12"/>
<connect gate="B" pin="PRE" pad="7"/>
<connect gate="B" pin="Q" pad="11"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*77" prefix="IC">
<description>4-bit D &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7477"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="12C" pad="12"/>
<connect gate="A" pin="1D" pad="1"/>
<connect gate="A" pin="1Q" pad="14"/>
<connect gate="A" pin="2D" pad="2"/>
<connect gate="A" pin="2Q" pad="13"/>
<connect gate="A" pin="34C" pad="3"/>
<connect gate="A" pin="3D" pad="5"/>
<connect gate="A" pin="3Q" pad="9"/>
<connect gate="A" pin="4D" pad="6"/>
<connect gate="A" pin="4Q" pad="8"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*78" prefix="IC">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset, common clock and common clear</description>
<gates>
<gate name="A" symbol="7478"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q1" pad="12"/>
<connect gate="A" pin="!Q2" pad="9"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="5"/>
<connect gate="A" pin="J1" pad="3"/>
<connect gate="A" pin="J2" pad="10"/>
<connect gate="A" pin="K1" pad="14"/>
<connect gate="A" pin="K2" pad="7"/>
<connect gate="A" pin="PR1" pad="2"/>
<connect gate="A" pin="PR2" pad="6"/>
<connect gate="A" pin="Q1" pad="13"/>
<connect gate="A" pin="Q2" pad="8"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*82" prefix="IC">
<description>2-bit binary full &lt;b&gt;ADDER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7482"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="14"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B2" pad="13"/>
<connect gate="A" pin="C0" pad="5"/>
<connect gate="A" pin="C2" pad="10"/>
<connect gate="A" pin="S1" pad="1"/>
<connect gate="A" pin="S2" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*83" prefix="IC">
<description>4-bit binary full &lt;b&gt;ADDER&lt;/b&gt;, fast carry</description>
<gates>
<gate name="A" symbol="7483"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="10"/>
<connect gate="A" pin="A2" pad="8"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="1"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="7"/>
<connect gate="A" pin="B3" pad="4"/>
<connect gate="A" pin="B4" pad="16"/>
<connect gate="A" pin="C0" pad="13"/>
<connect gate="A" pin="C4" pad="14"/>
<connect gate="A" pin="S1" pad="9"/>
<connect gate="A" pin="S2" pad="6"/>
<connect gate="A" pin="S3" pad="2"/>
<connect gate="A" pin="S4" pad="15"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*85" prefix="IC">
<description>4-bit magnitude &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7485"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A0" pad="10"/>
<connect gate="A" pin="A1" pad="12"/>
<connect gate="A" pin="A2" pad="13"/>
<connect gate="A" pin="A3" pad="15"/>
<connect gate="A" pin="A&lt;B_I" pad="2"/>
<connect gate="A" pin="A&lt;B_O" pad="7"/>
<connect gate="A" pin="A=B_I" pad="3"/>
<connect gate="A" pin="A=B_O" pad="6"/>
<connect gate="A" pin="A&gt;B_I" pad="4"/>
<connect gate="A" pin="A&gt;B_O" pad="5"/>
<connect gate="A" pin="B0" pad="9"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="14"/>
<connect gate="A" pin="B3" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A0" pad="10"/>
<connect gate="A" pin="A1" pad="12"/>
<connect gate="A" pin="A2" pad="13"/>
<connect gate="A" pin="A3" pad="15"/>
<connect gate="A" pin="A&lt;B_I" pad="2"/>
<connect gate="A" pin="A&lt;B_O" pad="7"/>
<connect gate="A" pin="A=B_I" pad="3"/>
<connect gate="A" pin="A=B_O" pad="6"/>
<connect gate="A" pin="A&gt;B_I" pad="4"/>
<connect gate="A" pin="A&gt;B_O" pad="5"/>
<connect gate="A" pin="B0" pad="9"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="14"/>
<connect gate="A" pin="B3" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A0" pad="13"/>
<connect gate="A" pin="A1" pad="15"/>
<connect gate="A" pin="A2" pad="17"/>
<connect gate="A" pin="A3" pad="19"/>
<connect gate="A" pin="A&lt;B_I" pad="3"/>
<connect gate="A" pin="A&lt;B_O" pad="9"/>
<connect gate="A" pin="A=B_I" pad="4"/>
<connect gate="A" pin="A=B_O" pad="8"/>
<connect gate="A" pin="A&gt;B_I" pad="5"/>
<connect gate="A" pin="A&gt;B_O" pad="7"/>
<connect gate="A" pin="B0" pad="12"/>
<connect gate="A" pin="B1" pad="14"/>
<connect gate="A" pin="B2" pad="18"/>
<connect gate="A" pin="B3" pad="2"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*90" prefix="IC">
<description>Decade, divide by twelve and binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7490"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="CKA" pad="14"/>
<connect gate="A" pin="CKB" pad="1"/>
<connect gate="A" pin="QA" pad="12"/>
<connect gate="A" pin="QB" pad="9"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="R0(1)" pad="2"/>
<connect gate="A" pin="R0(2)" pad="3"/>
<connect gate="A" pin="R9(1)" pad="6"/>
<connect gate="A" pin="R9(2)" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="CKA" pad="14"/>
<connect gate="A" pin="CKB" pad="1"/>
<connect gate="A" pin="QA" pad="12"/>
<connect gate="A" pin="QB" pad="9"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="R0(1)" pad="2"/>
<connect gate="A" pin="R0(2)" pad="3"/>
<connect gate="A" pin="R9(1)" pad="6"/>
<connect gate="A" pin="R9(2)" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*91" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7491"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!QH" pad="14"/>
<connect gate="A" pin="A" pad="12"/>
<connect gate="A" pin="B" pad="11"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="QH" pad="13"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*92" prefix="IC">
<description>Decade, divide by twelve and binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7492"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="CKA" pad="14"/>
<connect gate="A" pin="CKB" pad="1"/>
<connect gate="A" pin="QA" pad="12"/>
<connect gate="A" pin="QB" pad="11"/>
<connect gate="A" pin="QC" pad="9"/>
<connect gate="A" pin="QD" pad="8"/>
<connect gate="A" pin="R0(1)" pad="6"/>
<connect gate="A" pin="R0(2)" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="CKA" pad="14"/>
<connect gate="A" pin="CKB" pad="1"/>
<connect gate="A" pin="QA" pad="12"/>
<connect gate="A" pin="QB" pad="11"/>
<connect gate="A" pin="QC" pad="9"/>
<connect gate="A" pin="QD" pad="8"/>
<connect gate="A" pin="R0(1)" pad="6"/>
<connect gate="A" pin="R0(2)" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*93" prefix="IC">
<description>Decade, divide by twelve and binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7493"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="CKA" pad="14"/>
<connect gate="A" pin="CKB" pad="1"/>
<connect gate="A" pin="QA" pad="12"/>
<connect gate="A" pin="QB" pad="9"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="R0(1)" pad="2"/>
<connect gate="A" pin="R0(2)" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="CKA" pad="14"/>
<connect gate="A" pin="CKB" pad="1"/>
<connect gate="A" pin="QA" pad="12"/>
<connect gate="A" pin="QB" pad="9"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="R0(1)" pad="2"/>
<connect gate="A" pin="R0(2)" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*95" prefix="IC">
<description>4-bit parallel access &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7495"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="CK1" pad="9"/>
<connect gate="A" pin="CK2" pad="8"/>
<connect gate="A" pin="D" pad="5"/>
<connect gate="A" pin="MOD" pad="6"/>
<connect gate="A" pin="QA" pad="13"/>
<connect gate="A" pin="QB" pad="12"/>
<connect gate="A" pin="QC" pad="11"/>
<connect gate="A" pin="QD" pad="10"/>
<connect gate="A" pin="SER" pad="1"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*96" prefix="IC">
<description>5-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7496"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="16"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="E" pad="7"/>
<connect gate="A" pin="PE" pad="8"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="QE" pad="10"/>
<connect gate="A" pin="SER" pad="9"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="16"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="E" pad="7"/>
<connect gate="A" pin="PE" pad="8"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="QE" pad="10"/>
<connect gate="A" pin="SER" pad="9"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*97" prefix="IC">
<description>Synchronous 6-bit binary rate &lt;b&gt;MULTIPLIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7497"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="B0" pad="4"/>
<connect gate="A" pin="B1" pad="1"/>
<connect gate="A" pin="B2" pad="14"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="2"/>
<connect gate="A" pin="B5" pad="3"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="EI" pad="11"/>
<connect gate="A" pin="EO" pad="7"/>
<connect gate="A" pin="STR" pad="10"/>
<connect gate="A" pin="U/C" pad="12"/>
<connect gate="A" pin="Y" pad="6"/>
<connect gate="A" pin="Z" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="B0" pad="4"/>
<connect gate="A" pin="B1" pad="1"/>
<connect gate="A" pin="B2" pad="14"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="2"/>
<connect gate="A" pin="B5" pad="3"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="EI" pad="11"/>
<connect gate="A" pin="EO" pad="7"/>
<connect gate="A" pin="STR" pad="10"/>
<connect gate="A" pin="U/C" pad="12"/>
<connect gate="A" pin="Y" pad="6"/>
<connect gate="A" pin="Z" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*100" prefix="IC">
<description>8-bit bistable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74100"/>
<gate name="B" symbol="74100"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="D1" pad="2"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="22"/>
<connect gate="A" pin="D4" pad="21"/>
<connect gate="A" pin="EN" pad="23"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="4"/>
<connect gate="A" pin="Q3" pad="19"/>
<connect gate="A" pin="Q4" pad="20"/>
<connect gate="B" pin="D1" pad="11"/>
<connect gate="B" pin="D2" pad="10"/>
<connect gate="B" pin="D3" pad="15"/>
<connect gate="B" pin="D4" pad="16"/>
<connect gate="B" pin="EN" pad="12"/>
<connect gate="B" pin="Q1" pad="8"/>
<connect gate="B" pin="Q2" pad="9"/>
<connect gate="B" pin="Q3" pad="18"/>
<connect gate="B" pin="Q4" pad="17"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*107" prefix="IC">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="A" symbol="74107"/>
<gate name="B" symbol="74107"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="2"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="J" pad="1"/>
<connect gate="A" pin="K" pad="4"/>
<connect gate="A" pin="Q" pad="3"/>
<connect gate="B" pin="!Q" pad="6"/>
<connect gate="B" pin="CLK" pad="9"/>
<connect gate="B" pin="CLR" pad="10"/>
<connect gate="B" pin="J" pad="8"/>
<connect gate="B" pin="K" pad="11"/>
<connect gate="B" pin="Q" pad="5"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="!Q" pad="2"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="J" pad="1"/>
<connect gate="A" pin="K" pad="4"/>
<connect gate="A" pin="Q" pad="3"/>
<connect gate="B" pin="!Q" pad="6"/>
<connect gate="B" pin="CLK" pad="9"/>
<connect gate="B" pin="CLR" pad="10"/>
<connect gate="B" pin="J" pad="8"/>
<connect gate="B" pin="K" pad="11"/>
<connect gate="B" pin="Q" pad="5"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*109" prefix="IC">
<description>Dual J-K positive edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="A" symbol="74109"/>
<gate name="B" symbol="74109"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q" pad="7"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="J" pad="2"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="PRE" pad="5"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="B" pin="!Q" pad="9"/>
<connect gate="B" pin="CLK" pad="12"/>
<connect gate="B" pin="CLR" pad="15"/>
<connect gate="B" pin="J" pad="14"/>
<connect gate="B" pin="K" pad="13"/>
<connect gate="B" pin="PRE" pad="11"/>
<connect gate="B" pin="Q" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q" pad="7"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="J" pad="2"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="PRE" pad="5"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="B" pin="!Q" pad="9"/>
<connect gate="B" pin="CLK" pad="12"/>
<connect gate="B" pin="CLR" pad="15"/>
<connect gate="B" pin="J" pad="14"/>
<connect gate="B" pin="K" pad="13"/>
<connect gate="B" pin="PRE" pad="11"/>
<connect gate="B" pin="Q" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!Q" pad="9"/>
<connect gate="A" pin="CLK" pad="5"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="J" pad="3"/>
<connect gate="A" pin="K" pad="4"/>
<connect gate="A" pin="PRE" pad="7"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="B" pin="!Q" pad="12"/>
<connect gate="B" pin="CLK" pad="15"/>
<connect gate="B" pin="CLR" pad="19"/>
<connect gate="B" pin="J" pad="18"/>
<connect gate="B" pin="K" pad="17"/>
<connect gate="B" pin="PRE" pad="14"/>
<connect gate="B" pin="Q" pad="13"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*111" prefix="IC">
<description>Dual J-K master slave &lt;b&gt;FLIP FLOP&lt;/b&gt;, data lockout</description>
<gates>
<gate name="A" symbol="74111"/>
<gate name="B" symbol="74111"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="CLK" pad="5"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="J" pad="4"/>
<connect gate="A" pin="K" pad="1"/>
<connect gate="A" pin="PRE" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="B" pin="!Q" pad="10"/>
<connect gate="B" pin="CLK" pad="11"/>
<connect gate="B" pin="CLR" pad="13"/>
<connect gate="B" pin="J" pad="12"/>
<connect gate="B" pin="K" pad="15"/>
<connect gate="B" pin="PRE" pad="14"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*112" prefix="IC">
<description>Dual J-K negative edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="A" symbol="74112"/>
<gate name="B" symbol="74112"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="15"/>
<connect gate="A" pin="J" pad="3"/>
<connect gate="A" pin="K" pad="2"/>
<connect gate="A" pin="PRE" pad="4"/>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="B" pin="!Q" pad="7"/>
<connect gate="B" pin="CLK" pad="13"/>
<connect gate="B" pin="CLR" pad="14"/>
<connect gate="B" pin="J" pad="11"/>
<connect gate="B" pin="K" pad="12"/>
<connect gate="B" pin="PRE" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="15"/>
<connect gate="A" pin="J" pad="3"/>
<connect gate="A" pin="K" pad="2"/>
<connect gate="A" pin="PRE" pad="4"/>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="B" pin="!Q" pad="7"/>
<connect gate="B" pin="CLK" pad="13"/>
<connect gate="B" pin="CLR" pad="14"/>
<connect gate="B" pin="J" pad="11"/>
<connect gate="B" pin="K" pad="12"/>
<connect gate="B" pin="PRE" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!Q" pad="8"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="CLR" pad="19"/>
<connect gate="A" pin="J" pad="4"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="PRE" pad="5"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="B" pin="!Q" pad="9"/>
<connect gate="B" pin="CLK" pad="17"/>
<connect gate="B" pin="CLR" pad="18"/>
<connect gate="B" pin="J" pad="14"/>
<connect gate="B" pin="K" pad="15"/>
<connect gate="B" pin="PRE" pad="13"/>
<connect gate="B" pin="Q" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*113" prefix="IC">
<description>Dual J-K negative edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset</description>
<gates>
<gate name="A" symbol="74113"/>
<gate name="B" symbol="74113"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="J" pad="3"/>
<connect gate="A" pin="K" pad="2"/>
<connect gate="A" pin="PRE" pad="4"/>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="B" pin="!Q" pad="8"/>
<connect gate="B" pin="CLK" pad="13"/>
<connect gate="B" pin="J" pad="11"/>
<connect gate="B" pin="K" pad="12"/>
<connect gate="B" pin="PRE" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*114" prefix="IC">
<description>Dual J-K negative edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset, common clear, clock</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G$1" symbol="7478"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="G$1" pin="!Q1" pad="6"/>
<connect gate="G$1" pin="!Q2" pad="8"/>
<connect gate="G$1" pin="CLK" pad="13"/>
<connect gate="G$1" pin="CLR" pad="1"/>
<connect gate="G$1" pin="J1" pad="3"/>
<connect gate="G$1" pin="J2" pad="11"/>
<connect gate="G$1" pin="K1" pad="2"/>
<connect gate="G$1" pin="K2" pad="12"/>
<connect gate="G$1" pin="PR1" pad="4"/>
<connect gate="G$1" pin="PR2" pad="10"/>
<connect gate="G$1" pin="Q1" pad="5"/>
<connect gate="G$1" pin="Q2" pad="9"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*116" prefix="IC">
<description>Dual 4-bit &lt;b&gt;LATCH&lt;/b&gt; with clear</description>
<gates>
<gate name="A" symbol="74116"/>
<gate name="B" symbol="74116"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="10"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="11"/>
<connect gate="B" pin="CLR" pad="13"/>
<connect gate="B" pin="D1" pad="16"/>
<connect gate="B" pin="D2" pad="18"/>
<connect gate="B" pin="D3" pad="20"/>
<connect gate="B" pin="D4" pad="22"/>
<connect gate="B" pin="G1" pad="14"/>
<connect gate="B" pin="G2" pad="15"/>
<connect gate="B" pin="Q1" pad="17"/>
<connect gate="B" pin="Q2" pad="19"/>
<connect gate="B" pin="Q3" pad="21"/>
<connect gate="B" pin="Q4" pad="23"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*120" prefix="IC">
<description>Dual pulse &lt;b&gt;SYNCHRONIZER/DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74120"/>
<gate name="B" symbol="74120"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Y" pad="7"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="M" pad="1"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="A" pin="Y" pad="6"/>
<connect gate="B" pin="!Y" pad="9"/>
<connect gate="B" pin="C" pad="11"/>
<connect gate="B" pin="M" pad="15"/>
<connect gate="B" pin="R" pad="12"/>
<connect gate="B" pin="S1" pad="13"/>
<connect gate="B" pin="S2" pad="14"/>
<connect gate="B" pin="Y" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*121" prefix="IC">
<description>Monostable &lt;b&gt;MULTIVIBRATOR&lt;/b&gt;, schmitt trigger inputs</description>
<gates>
<gate name="A" symbol="74121"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="A" pin="R" pad="9"/>
<connect gate="A" pin="R/C" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="!Q" pad="1"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="A" pin="R" pad="9"/>
<connect gate="A" pin="R/C" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*122" prefix="IC">
<description>Retriggerable monostable &lt;b&gt;MULTIVIBRATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74122"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B2" pad="4"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="CLR" pad="5"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="R" pad="9"/>
<connect gate="A" pin="R/C" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B2" pad="4"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="CLR" pad="5"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="R" pad="9"/>
<connect gate="A" pin="R/C" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*123" prefix="IC">
<description>Retriggerable monostable &lt;b&gt;MULTIVIBRATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74123"/>
<gate name="B" symbol="74123"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q" pad="4"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="Q" pad="13"/>
<connect gate="A" pin="R/C" pad="15"/>
<connect gate="B" pin="!Q" pad="12"/>
<connect gate="B" pin="A" pad="9"/>
<connect gate="B" pin="B" pad="10"/>
<connect gate="B" pin="C" pad="6"/>
<connect gate="B" pin="CLR" pad="11"/>
<connect gate="B" pin="Q" pad="5"/>
<connect gate="B" pin="R/C" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q" pad="4"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="Q" pad="13"/>
<connect gate="A" pin="R/C" pad="15"/>
<connect gate="B" pin="!Q" pad="12"/>
<connect gate="B" pin="A" pad="9"/>
<connect gate="B" pin="B" pad="10"/>
<connect gate="B" pin="C" pad="6"/>
<connect gate="B" pin="CLR" pad="11"/>
<connect gate="B" pin="Q" pad="5"/>
<connect gate="B" pin="R/C" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!Q" pad="5"/>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="18"/>
<connect gate="A" pin="CLR" pad="4"/>
<connect gate="A" pin="Q" pad="17"/>
<connect gate="A" pin="R/C" pad="19"/>
<connect gate="B" pin="!Q" pad="15"/>
<connect gate="B" pin="A" pad="12"/>
<connect gate="B" pin="B" pad="13"/>
<connect gate="B" pin="C" pad="8"/>
<connect gate="B" pin="CLR" pad="14"/>
<connect gate="B" pin="Q" pad="7"/>
<connect gate="B" pin="R/C" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*124" prefix="IC">
<description>Dual &lt;b&gt;VCO&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74124"/>
<gate name="B" symbol="74124"/>
<gate name="C" symbol="OSCPWR"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CX@1" pad="4"/>
<connect gate="A" pin="CX@2" pad="5"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="FC" pad="2"/>
<connect gate="A" pin="RNG" pad="3"/>
<connect gate="A" pin="Y" pad="7"/>
<connect gate="B" pin="CX@1" pad="12"/>
<connect gate="B" pin="CX@2" pad="13"/>
<connect gate="B" pin="EN" pad="11"/>
<connect gate="B" pin="FC" pad="1"/>
<connect gate="B" pin="RNG" pad="14"/>
<connect gate="B" pin="Y" pad="10"/>
<connect gate="C" pin="OSCGND" pad="8"/>
<connect gate="C" pin="OSCVCC" pad="15"/>
<connect gate="P" pin="GND" pad="9"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="CX@1" pad="4"/>
<connect gate="A" pin="CX@2" pad="5"/>
<connect gate="A" pin="EN" pad="6"/>
<connect gate="A" pin="FC" pad="2"/>
<connect gate="A" pin="RNG" pad="3"/>
<connect gate="A" pin="Y" pad="7"/>
<connect gate="B" pin="CX@1" pad="12"/>
<connect gate="B" pin="CX@2" pad="13"/>
<connect gate="B" pin="EN" pad="11"/>
<connect gate="B" pin="FC" pad="1"/>
<connect gate="B" pin="RNG" pad="14"/>
<connect gate="B" pin="Y" pad="10"/>
<connect gate="C" pin="OSCGND" pad="8"/>
<connect gate="C" pin="OSCVCC" pad="15"/>
<connect gate="P" pin="GND" pad="9"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="CX@1" pad="5"/>
<connect gate="A" pin="CX@2" pad="7"/>
<connect gate="A" pin="EN" pad="8"/>
<connect gate="A" pin="FC" pad="3"/>
<connect gate="A" pin="RNG" pad="4"/>
<connect gate="A" pin="Y" pad="9"/>
<connect gate="B" pin="CX@1" pad="15"/>
<connect gate="B" pin="CX@2" pad="17"/>
<connect gate="B" pin="EN" pad="14"/>
<connect gate="B" pin="FC" pad="2"/>
<connect gate="B" pin="RNG" pad="18"/>
<connect gate="B" pin="Y" pad="13"/>
<connect gate="C" pin="OSCGND" pad="10"/>
<connect gate="C" pin="OSCVCC" pad="19"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*131" prefix="IC">
<description>3-line to 8-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;, address register</description>
<gates>
<gate name="A" symbol="74131"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="G1" pad="6"/>
<connect gate="A" pin="G2" pad="5"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*137" prefix="IC">
<description>3-line to 8-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;, address LATCH</description>
<gates>
<gate name="A" symbol="74137"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="G1" pad="6"/>
<connect gate="A" pin="G2" pad="5"/>
<connect gate="A" pin="GL" pad="4"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="G1" pad="6"/>
<connect gate="A" pin="G2" pad="5"/>
<connect gate="A" pin="GL" pad="4"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="G1" pad="8"/>
<connect gate="A" pin="G2" pad="7"/>
<connect gate="A" pin="GL" pad="5"/>
<connect gate="A" pin="Y0" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="15"/>
<connect gate="A" pin="Y4" pad="14"/>
<connect gate="A" pin="Y5" pad="13"/>
<connect gate="A" pin="Y6" pad="12"/>
<connect gate="A" pin="Y7" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*138" prefix="IC">
<description>3-line to 8-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74138"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="G1" pad="6"/>
<connect gate="A" pin="G2A" pad="4"/>
<connect gate="A" pin="G2B" pad="5"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="G1" pad="6"/>
<connect gate="A" pin="G2A" pad="4"/>
<connect gate="A" pin="G2B" pad="5"/>
<connect gate="A" pin="Y0" pad="15"/>
<connect gate="A" pin="Y1" pad="14"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="10"/>
<connect gate="A" pin="Y6" pad="9"/>
<connect gate="A" pin="Y7" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="G1" pad="8"/>
<connect gate="A" pin="G2A" pad="5"/>
<connect gate="A" pin="G2B" pad="7"/>
<connect gate="A" pin="Y0" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="15"/>
<connect gate="A" pin="Y4" pad="14"/>
<connect gate="A" pin="Y5" pad="13"/>
<connect gate="A" pin="Y6" pad="12"/>
<connect gate="A" pin="Y7" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*139" prefix="IC">
<description>Dual 2-line to 4-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74139"/>
<gate name="B" symbol="74139"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y0" pad="4"/>
<connect gate="A" pin="Y1" pad="5"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="B" pin="A" pad="14"/>
<connect gate="B" pin="B" pad="13"/>
<connect gate="B" pin="G" pad="15"/>
<connect gate="B" pin="Y0" pad="12"/>
<connect gate="B" pin="Y1" pad="11"/>
<connect gate="B" pin="Y2" pad="10"/>
<connect gate="B" pin="Y3" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y0" pad="4"/>
<connect gate="A" pin="Y1" pad="5"/>
<connect gate="A" pin="Y2" pad="6"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="B" pin="A" pad="14"/>
<connect gate="B" pin="B" pad="13"/>
<connect gate="B" pin="G" pad="15"/>
<connect gate="B" pin="Y0" pad="12"/>
<connect gate="B" pin="Y1" pad="11"/>
<connect gate="B" pin="Y2" pad="10"/>
<connect gate="B" pin="Y3" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="G" pad="2"/>
<connect gate="A" pin="Y0" pad="5"/>
<connect gate="A" pin="Y1" pad="7"/>
<connect gate="A" pin="Y2" pad="8"/>
<connect gate="A" pin="Y3" pad="9"/>
<connect gate="B" pin="A" pad="18"/>
<connect gate="B" pin="B" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y0" pad="15"/>
<connect gate="B" pin="Y1" pad="14"/>
<connect gate="B" pin="Y2" pad="13"/>
<connect gate="B" pin="Y3" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*143" prefix="IC">
<description>4-bit &lt;b&gt;COUNTER/LATCH SEVEN-SEGMENT LED/LAMP DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74143"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="16"/>
<connect gate="A" pin="BI" pad="5"/>
<connect gate="A" pin="BI/RBO" pad="6"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="DP@2" pad="8"/>
<connect gate="A" pin="DPI" pad="7"/>
<connect gate="A" pin="DPO" pad="22"/>
<connect gate="A" pin="E" pad="11"/>
<connect gate="A" pin="F" pad="10"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="PCEI" pad="23"/>
<connect gate="A" pin="QA" pad="17"/>
<connect gate="A" pin="QB" pad="18"/>
<connect gate="A" pin="QC" pad="19"/>
<connect gate="A" pin="QD" pad="20"/>
<connect gate="A" pin="RBI" pad="4"/>
<connect gate="A" pin="SCEI" pad="1"/>
<connect gate="A" pin="STR" pad="21"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*145" prefix="IC">
<description>BCD to decimal &lt;b&gt;DECODER/DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74145"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="0" pad="1"/>
<connect gate="A" pin="1" pad="2"/>
<connect gate="A" pin="2" pad="3"/>
<connect gate="A" pin="3" pad="4"/>
<connect gate="A" pin="4" pad="5"/>
<connect gate="A" pin="5" pad="6"/>
<connect gate="A" pin="6" pad="7"/>
<connect gate="A" pin="7" pad="9"/>
<connect gate="A" pin="8" pad="10"/>
<connect gate="A" pin="9" pad="11"/>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="0" pad="1"/>
<connect gate="A" pin="1" pad="2"/>
<connect gate="A" pin="2" pad="3"/>
<connect gate="A" pin="3" pad="4"/>
<connect gate="A" pin="4" pad="5"/>
<connect gate="A" pin="5" pad="6"/>
<connect gate="A" pin="6" pad="7"/>
<connect gate="A" pin="7" pad="9"/>
<connect gate="A" pin="8" pad="10"/>
<connect gate="A" pin="9" pad="11"/>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="0" pad="2"/>
<connect gate="A" pin="1" pad="3"/>
<connect gate="A" pin="2" pad="4"/>
<connect gate="A" pin="3" pad="5"/>
<connect gate="A" pin="4" pad="7"/>
<connect gate="A" pin="5" pad="8"/>
<connect gate="A" pin="6" pad="9"/>
<connect gate="A" pin="7" pad="12"/>
<connect gate="A" pin="8" pad="13"/>
<connect gate="A" pin="9" pad="14"/>
<connect gate="A" pin="A" pad="19"/>
<connect gate="A" pin="B" pad="18"/>
<connect gate="A" pin="C" pad="17"/>
<connect gate="A" pin="D" pad="15"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*147" prefix="IC">
<description>10-line to 4-line and 8-line to 3-line &lt;b&gt;PRIORITY DECODER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74147"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1" pad="11"/>
<connect gate="A" pin="2" pad="12"/>
<connect gate="A" pin="3" pad="13"/>
<connect gate="A" pin="4" pad="1"/>
<connect gate="A" pin="5" pad="2"/>
<connect gate="A" pin="6" pad="3"/>
<connect gate="A" pin="7" pad="4"/>
<connect gate="A" pin="8" pad="5"/>
<connect gate="A" pin="9" pad="10"/>
<connect gate="A" pin="A" pad="9"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="C" pad="6"/>
<connect gate="A" pin="D" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*148" prefix="IC">
<description>10-line to 4-line and 8-line to 3-line &lt;b&gt;PRIORITY ENCODER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74148"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="0" pad="10"/>
<connect gate="A" pin="1" pad="11"/>
<connect gate="A" pin="2" pad="12"/>
<connect gate="A" pin="3" pad="13"/>
<connect gate="A" pin="4" pad="1"/>
<connect gate="A" pin="5" pad="2"/>
<connect gate="A" pin="6" pad="3"/>
<connect gate="A" pin="7" pad="4"/>
<connect gate="A" pin="A0" pad="9"/>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A2" pad="6"/>
<connect gate="A" pin="EI" pad="5"/>
<connect gate="A" pin="EO" pad="15"/>
<connect gate="A" pin="GS" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="0" pad="10"/>
<connect gate="A" pin="1" pad="11"/>
<connect gate="A" pin="2" pad="12"/>
<connect gate="A" pin="3" pad="13"/>
<connect gate="A" pin="4" pad="1"/>
<connect gate="A" pin="5" pad="2"/>
<connect gate="A" pin="6" pad="3"/>
<connect gate="A" pin="7" pad="4"/>
<connect gate="A" pin="A0" pad="9"/>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A2" pad="6"/>
<connect gate="A" pin="EI" pad="5"/>
<connect gate="A" pin="EO" pad="15"/>
<connect gate="A" pin="GS" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="0" pad="13"/>
<connect gate="A" pin="1" pad="14"/>
<connect gate="A" pin="2" pad="15"/>
<connect gate="A" pin="3" pad="17"/>
<connect gate="A" pin="4" pad="2"/>
<connect gate="A" pin="5" pad="3"/>
<connect gate="A" pin="6" pad="4"/>
<connect gate="A" pin="7" pad="5"/>
<connect gate="A" pin="A0" pad="12"/>
<connect gate="A" pin="A1" pad="9"/>
<connect gate="A" pin="A2" pad="8"/>
<connect gate="A" pin="EI" pad="7"/>
<connect gate="A" pin="EO" pad="19"/>
<connect gate="A" pin="GS" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*150" prefix="IC">
<description>Data &lt;B&gt;SELCTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74150"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="11"/>
<connect gate="A" pin="E0" pad="8"/>
<connect gate="A" pin="E1" pad="7"/>
<connect gate="A" pin="E10" pad="21"/>
<connect gate="A" pin="E11" pad="20"/>
<connect gate="A" pin="E12" pad="19"/>
<connect gate="A" pin="E13" pad="18"/>
<connect gate="A" pin="E14" pad="17"/>
<connect gate="A" pin="E15" pad="16"/>
<connect gate="A" pin="E2" pad="6"/>
<connect gate="A" pin="E3" pad="5"/>
<connect gate="A" pin="E4" pad="4"/>
<connect gate="A" pin="E5" pad="3"/>
<connect gate="A" pin="E6" pad="2"/>
<connect gate="A" pin="E7" pad="1"/>
<connect gate="A" pin="E8" pad="23"/>
<connect gate="A" pin="E9" pad="22"/>
<connect gate="A" pin="G" pad="9"/>
<connect gate="A" pin="W" pad="10"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*151" prefix="IC">
<description>Data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74151"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="D0" pad="4"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="2"/>
<connect gate="A" pin="D3" pad="1"/>
<connect gate="A" pin="D4" pad="15"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="13"/>
<connect gate="A" pin="D7" pad="12"/>
<connect gate="A" pin="G" pad="7"/>
<connect gate="A" pin="W" pad="6"/>
<connect gate="A" pin="Y" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="D0" pad="4"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="2"/>
<connect gate="A" pin="D3" pad="1"/>
<connect gate="A" pin="D4" pad="15"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="13"/>
<connect gate="A" pin="D7" pad="12"/>
<connect gate="A" pin="G" pad="7"/>
<connect gate="A" pin="W" pad="6"/>
<connect gate="A" pin="Y" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="13"/>
<connect gate="A" pin="C" pad="12"/>
<connect gate="A" pin="D0" pad="5"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="19"/>
<connect gate="A" pin="D5" pad="18"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="15"/>
<connect gate="A" pin="G" pad="9"/>
<connect gate="A" pin="W" pad="8"/>
<connect gate="A" pin="Y" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*152" prefix="IC">
<description>Data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74152"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="C" pad="8"/>
<connect gate="A" pin="D0" pad="5"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="1"/>
<connect gate="A" pin="D5" pad="13"/>
<connect gate="A" pin="D6" pad="12"/>
<connect gate="A" pin="D7" pad="11"/>
<connect gate="A" pin="W" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*153" prefix="IC">
<description>Dual 4-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74153"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1C0" pad="6"/>
<connect gate="A" pin="1C1" pad="5"/>
<connect gate="A" pin="1C2" pad="4"/>
<connect gate="A" pin="1C3" pad="3"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y" pad="7"/>
<connect gate="A" pin="2C0" pad="10"/>
<connect gate="A" pin="2C1" pad="11"/>
<connect gate="A" pin="2C2" pad="12"/>
<connect gate="A" pin="2C3" pad="13"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C0" pad="6"/>
<connect gate="A" pin="1C1" pad="5"/>
<connect gate="A" pin="1C2" pad="4"/>
<connect gate="A" pin="1C3" pad="3"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y" pad="7"/>
<connect gate="A" pin="2C0" pad="10"/>
<connect gate="A" pin="2C1" pad="11"/>
<connect gate="A" pin="2C2" pad="12"/>
<connect gate="A" pin="2C3" pad="13"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1C0" pad="8"/>
<connect gate="A" pin="1C1" pad="7"/>
<connect gate="A" pin="1C2" pad="5"/>
<connect gate="A" pin="1C3" pad="4"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y" pad="9"/>
<connect gate="A" pin="2C0" pad="13"/>
<connect gate="A" pin="2C1" pad="14"/>
<connect gate="A" pin="2C2" pad="15"/>
<connect gate="A" pin="2C3" pad="17"/>
<connect gate="A" pin="2G" pad="19"/>
<connect gate="A" pin="2Y" pad="12"/>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*154" prefix="IC">
<description>4-line to 16-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74154"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="0" pad="1"/>
<connect gate="A" pin="1" pad="2"/>
<connect gate="A" pin="10" pad="11"/>
<connect gate="A" pin="11" pad="13"/>
<connect gate="A" pin="12" pad="14"/>
<connect gate="A" pin="13" pad="15"/>
<connect gate="A" pin="14" pad="16"/>
<connect gate="A" pin="15" pad="17"/>
<connect gate="A" pin="2" pad="3"/>
<connect gate="A" pin="3" pad="4"/>
<connect gate="A" pin="4" pad="5"/>
<connect gate="A" pin="5" pad="6"/>
<connect gate="A" pin="6" pad="7"/>
<connect gate="A" pin="7" pad="8"/>
<connect gate="A" pin="8" pad="9"/>
<connect gate="A" pin="9" pad="10"/>
<connect gate="A" pin="A" pad="23"/>
<connect gate="A" pin="B" pad="22"/>
<connect gate="A" pin="C" pad="21"/>
<connect gate="A" pin="D" pad="20"/>
<connect gate="A" pin="G1" pad="18"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DW" package="SO24W">
<connects>
<connect gate="A" pin="0" pad="1"/>
<connect gate="A" pin="1" pad="2"/>
<connect gate="A" pin="10" pad="11"/>
<connect gate="A" pin="11" pad="13"/>
<connect gate="A" pin="12" pad="14"/>
<connect gate="A" pin="13" pad="15"/>
<connect gate="A" pin="14" pad="16"/>
<connect gate="A" pin="15" pad="17"/>
<connect gate="A" pin="2" pad="3"/>
<connect gate="A" pin="3" pad="4"/>
<connect gate="A" pin="4" pad="5"/>
<connect gate="A" pin="5" pad="6"/>
<connect gate="A" pin="6" pad="7"/>
<connect gate="A" pin="7" pad="8"/>
<connect gate="A" pin="8" pad="9"/>
<connect gate="A" pin="9" pad="10"/>
<connect gate="A" pin="A" pad="23"/>
<connect gate="A" pin="B" pad="22"/>
<connect gate="A" pin="C" pad="21"/>
<connect gate="A" pin="D" pad="20"/>
<connect gate="A" pin="G1" pad="18"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*155" prefix="IC">
<description>Dual 2-line to 4-line data &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74155"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1C" pad="1"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y0" pad="7"/>
<connect gate="A" pin="1Y1" pad="6"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="4"/>
<connect gate="A" pin="2C" pad="15"/>
<connect gate="A" pin="2G" pad="14"/>
<connect gate="A" pin="2Y0" pad="9"/>
<connect gate="A" pin="2Y1" pad="10"/>
<connect gate="A" pin="2Y2" pad="11"/>
<connect gate="A" pin="2Y3" pad="12"/>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C" pad="1"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y0" pad="7"/>
<connect gate="A" pin="1Y1" pad="6"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="4"/>
<connect gate="A" pin="2C" pad="15"/>
<connect gate="A" pin="2G" pad="14"/>
<connect gate="A" pin="2Y0" pad="9"/>
<connect gate="A" pin="2Y1" pad="10"/>
<connect gate="A" pin="2Y2" pad="11"/>
<connect gate="A" pin="2Y3" pad="12"/>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1C" pad="2"/>
<connect gate="A" pin="1G" pad="3"/>
<connect gate="A" pin="1Y0" pad="9"/>
<connect gate="A" pin="1Y1" pad="8"/>
<connect gate="A" pin="1Y2" pad="7"/>
<connect gate="A" pin="1Y3" pad="5"/>
<connect gate="A" pin="2C" pad="19"/>
<connect gate="A" pin="2G" pad="18"/>
<connect gate="A" pin="2Y0" pad="12"/>
<connect gate="A" pin="2Y1" pad="13"/>
<connect gate="A" pin="2Y2" pad="14"/>
<connect gate="A" pin="2Y3" pad="15"/>
<connect gate="A" pin="A" pad="17"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*156" prefix="IC">
<description>Dual 2-line to 4-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74156"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1C" pad="1"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y0" pad="7"/>
<connect gate="A" pin="1Y1" pad="6"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="4"/>
<connect gate="A" pin="2C" pad="15"/>
<connect gate="A" pin="2G" pad="14"/>
<connect gate="A" pin="2Y0" pad="9"/>
<connect gate="A" pin="2Y1" pad="10"/>
<connect gate="A" pin="2Y2" pad="11"/>
<connect gate="A" pin="2Y3" pad="12"/>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C" pad="1"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y0" pad="7"/>
<connect gate="A" pin="1Y1" pad="6"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="4"/>
<connect gate="A" pin="2C" pad="15"/>
<connect gate="A" pin="2G" pad="14"/>
<connect gate="A" pin="2Y0" pad="9"/>
<connect gate="A" pin="2Y1" pad="10"/>
<connect gate="A" pin="2Y2" pad="11"/>
<connect gate="A" pin="2Y3" pad="12"/>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1C" pad="2"/>
<connect gate="A" pin="1G" pad="3"/>
<connect gate="A" pin="1Y0" pad="9"/>
<connect gate="A" pin="1Y1" pad="8"/>
<connect gate="A" pin="1Y2" pad="7"/>
<connect gate="A" pin="1Y3" pad="5"/>
<connect gate="A" pin="2C" pad="19"/>
<connect gate="A" pin="2G" pad="18"/>
<connect gate="A" pin="2Y0" pad="12"/>
<connect gate="A" pin="2Y1" pad="13"/>
<connect gate="A" pin="2Y2" pad="14"/>
<connect gate="A" pin="2Y3" pad="15"/>
<connect gate="A" pin="A" pad="17"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*157" prefix="IC">
<description>Quadruple 2-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74157"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!A!/B" pad="2"/>
<connect gate="A" pin="1A" pad="3"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1Y" pad="5"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="4A" pad="18"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4Y" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*158" prefix="IC">
<description>Quadruple 2-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74158"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!A!/B" pad="2"/>
<connect gate="A" pin="1A" pad="3"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1Y" pad="5"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="4A" pad="18"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4Y" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*159" prefix="IC">
<description>4-line to 16-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="74159"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="0" pad="1"/>
<connect gate="A" pin="1" pad="2"/>
<connect gate="A" pin="10" pad="11"/>
<connect gate="A" pin="11" pad="13"/>
<connect gate="A" pin="12" pad="14"/>
<connect gate="A" pin="13" pad="15"/>
<connect gate="A" pin="14" pad="16"/>
<connect gate="A" pin="15" pad="17"/>
<connect gate="A" pin="2" pad="3"/>
<connect gate="A" pin="3" pad="4"/>
<connect gate="A" pin="4" pad="5"/>
<connect gate="A" pin="5" pad="6"/>
<connect gate="A" pin="6" pad="7"/>
<connect gate="A" pin="7" pad="8"/>
<connect gate="A" pin="8" pad="9"/>
<connect gate="A" pin="9" pad="10"/>
<connect gate="A" pin="A" pad="23"/>
<connect gate="A" pin="B" pad="22"/>
<connect gate="A" pin="C" pad="21"/>
<connect gate="A" pin="D" pad="20"/>
<connect gate="A" pin="G1" pad="18"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*160" prefix="IC">
<description>Synchronous 4-bit &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74160"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="10"/>
<connect gate="A" pin="LD" pad="9"/>
<connect gate="A" pin="QA" pad="14"/>
<connect gate="A" pin="QB" pad="13"/>
<connect gate="A" pin="QC" pad="12"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="RCO" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*164" prefix="IC">
<description>8-bit parallel out &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74164"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="CLK" pad="8"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="4"/>
<connect gate="A" pin="QC" pad="5"/>
<connect gate="A" pin="QD" pad="6"/>
<connect gate="A" pin="QE" pad="10"/>
<connect gate="A" pin="QF" pad="11"/>
<connect gate="A" pin="QG" pad="12"/>
<connect gate="A" pin="QH" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="CLK" pad="8"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="4"/>
<connect gate="A" pin="QC" pad="5"/>
<connect gate="A" pin="QD" pad="6"/>
<connect gate="A" pin="QE" pad="10"/>
<connect gate="A" pin="QF" pad="11"/>
<connect gate="A" pin="QG" pad="12"/>
<connect gate="A" pin="QH" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ABT"/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="QA" pad="4"/>
<connect gate="A" pin="QB" pad="6"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="A" pin="QE" pad="14"/>
<connect gate="A" pin="QF" pad="16"/>
<connect gate="A" pin="QG" pad="18"/>
<connect gate="A" pin="QH" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*165" prefix="IC">
<description>8-bit parallel load &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74165"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!QH" pad="7"/>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="D" pad="14"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="A" pin="F" pad="4"/>
<connect gate="A" pin="G" pad="5"/>
<connect gate="A" pin="H" pad="6"/>
<connect gate="A" pin="INH" pad="15"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="SER" pad="10"/>
<connect gate="A" pin="SH/!LD" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!QH" pad="7"/>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="12"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="D" pad="14"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="A" pin="F" pad="4"/>
<connect gate="A" pin="G" pad="5"/>
<connect gate="A" pin="H" pad="6"/>
<connect gate="A" pin="INH" pad="15"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="SER" pad="10"/>
<connect gate="A" pin="SH/!LD" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!QH" pad="9"/>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="15"/>
<connect gate="A" pin="C" pad="17"/>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="D" pad="18"/>
<connect gate="A" pin="E" pad="4"/>
<connect gate="A" pin="F" pad="5"/>
<connect gate="A" pin="G" pad="7"/>
<connect gate="A" pin="H" pad="8"/>
<connect gate="A" pin="INH" pad="19"/>
<connect gate="A" pin="QH" pad="12"/>
<connect gate="A" pin="SER" pad="13"/>
<connect gate="A" pin="SH/!LD" pad="2"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*166" prefix="IC">
<description>8-bit parallel load &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74166"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="D" pad="5"/>
<connect gate="A" pin="E" pad="10"/>
<connect gate="A" pin="F" pad="11"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="H" pad="14"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="QH" pad="13"/>
<connect gate="A" pin="SER" pad="1"/>
<connect gate="A" pin="SH/!LD" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="D" pad="5"/>
<connect gate="A" pin="E" pad="10"/>
<connect gate="A" pin="F" pad="11"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="H" pad="14"/>
<connect gate="A" pin="INH" pad="6"/>
<connect gate="A" pin="QH" pad="13"/>
<connect gate="A" pin="SER" pad="1"/>
<connect gate="A" pin="SH/!LD" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="12"/>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="E" pad="13"/>
<connect gate="A" pin="F" pad="14"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="A" pin="H" pad="18"/>
<connect gate="A" pin="INH" pad="8"/>
<connect gate="A" pin="QH" pad="17"/>
<connect gate="A" pin="SER" pad="2"/>
<connect gate="A" pin="SH/!LD" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*167" prefix="IC">
<description>Synchronous decade rate &lt;b&gt;MULTIPLIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74167"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="B0" pad="14"/>
<connect gate="A" pin="B1" pad="15"/>
<connect gate="A" pin="B2" pad="2"/>
<connect gate="A" pin="B3" pad="3"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="EI" pad="11"/>
<connect gate="A" pin="EO" pad="7"/>
<connect gate="A" pin="ST9" pad="4"/>
<connect gate="A" pin="STR" pad="10"/>
<connect gate="A" pin="U/C" pad="12"/>
<connect gate="A" pin="Y" pad="6"/>
<connect gate="A" pin="Z" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*168" prefix="IC">
<description>Synchronous 4-bit &lt;b&gt;UP/DOWN COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74168"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="10"/>
<connect gate="A" pin="LD" pad="9"/>
<connect gate="A" pin="QA" pad="14"/>
<connect gate="A" pin="QB" pad="13"/>
<connect gate="A" pin="QC" pad="12"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="RCO" pad="15"/>
<connect gate="A" pin="U/!D" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*170" prefix="IC">
<description>4 by 4 &lt;b&gt;REGISTER&lt;/b&gt; files, open collector</description>
<gates>
<gate name="A" symbol="74170"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D2" pad="1"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="3"/>
<connect gate="A" pin="GR" pad="11"/>
<connect gate="A" pin="GW" pad="12"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="6"/>
<connect gate="A" pin="RA" pad="5"/>
<connect gate="A" pin="RB" pad="4"/>
<connect gate="A" pin="WA" pad="14"/>
<connect gate="A" pin="WB" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D2" pad="1"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="3"/>
<connect gate="A" pin="GR" pad="11"/>
<connect gate="A" pin="GW" pad="12"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="6"/>
<connect gate="A" pin="RA" pad="5"/>
<connect gate="A" pin="RB" pad="4"/>
<connect gate="A" pin="WA" pad="14"/>
<connect gate="A" pin="WB" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="D1" pad="19"/>
<connect gate="A" pin="D2" pad="2"/>
<connect gate="A" pin="D3" pad="3"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="GR" pad="14"/>
<connect gate="A" pin="GW" pad="15"/>
<connect gate="A" pin="Q1" pad="13"/>
<connect gate="A" pin="Q2" pad="12"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="8"/>
<connect gate="A" pin="RA" pad="7"/>
<connect gate="A" pin="RB" pad="5"/>
<connect gate="A" pin="WA" pad="18"/>
<connect gate="A" pin="WB" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*171" prefix="IC">
<description>Quadruple D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="A" symbol="74171"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q1" pad="1"/>
<connect gate="A" pin="!Q2" pad="2"/>
<connect gate="A" pin="!Q3" pad="7"/>
<connect gate="A" pin="!Q4" pad="9"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="11"/>
<connect gate="A" pin="Q1" pad="15"/>
<connect gate="A" pin="Q2" pad="3"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*173" prefix="IC">
<description>4-bit D type &lt;b&gt;REGISTER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74173"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="CLR" pad="15"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D2" pad="13"/>
<connect gate="A" pin="D3" pad="12"/>
<connect gate="A" pin="D4" pad="11"/>
<connect gate="A" pin="G1" pad="9"/>
<connect gate="A" pin="G2" pad="10"/>
<connect gate="A" pin="M" pad="1"/>
<connect gate="A" pin="N" pad="2"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="4"/>
<connect gate="A" pin="Q3" pad="5"/>
<connect gate="A" pin="Q4" pad="6"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="CLR" pad="15"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D2" pad="13"/>
<connect gate="A" pin="D3" pad="12"/>
<connect gate="A" pin="D4" pad="11"/>
<connect gate="A" pin="G1" pad="9"/>
<connect gate="A" pin="G2" pad="10"/>
<connect gate="A" pin="M" pad="1"/>
<connect gate="A" pin="N" pad="2"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="4"/>
<connect gate="A" pin="Q3" pad="5"/>
<connect gate="A" pin="Q4" pad="6"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="19"/>
<connect gate="A" pin="D1" pad="18"/>
<connect gate="A" pin="D2" pad="17"/>
<connect gate="A" pin="D3" pad="15"/>
<connect gate="A" pin="D4" pad="14"/>
<connect gate="A" pin="G1" pad="12"/>
<connect gate="A" pin="G2" pad="13"/>
<connect gate="A" pin="M" pad="2"/>
<connect gate="A" pin="N" pad="3"/>
<connect gate="A" pin="Q1" pad="4"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="8"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*174" prefix="IC">
<description>Hex D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="A" symbol="74174"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="6"/>
<connect gate="A" pin="D4" pad="11"/>
<connect gate="A" pin="D5" pad="13"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="10"/>
<connect gate="A" pin="Q5" pad="12"/>
<connect gate="A" pin="Q6" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="6"/>
<connect gate="A" pin="D4" pad="11"/>
<connect gate="A" pin="D5" pad="13"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="10"/>
<connect gate="A" pin="Q5" pad="12"/>
<connect gate="A" pin="Q6" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="5"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="14"/>
<connect gate="A" pin="D5" pad="17"/>
<connect gate="A" pin="D6" pad="18"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="13"/>
<connect gate="A" pin="Q5" pad="15"/>
<connect gate="A" pin="Q6" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*175" prefix="IC">
<description>Qadruple D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="A" symbol="74175"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!Q1" pad="3"/>
<connect gate="A" pin="!Q2" pad="6"/>
<connect gate="A" pin="!Q3" pad="11"/>
<connect gate="A" pin="!Q4" pad="14"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="5"/>
<connect gate="A" pin="D3" pad="12"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="10"/>
<connect gate="A" pin="Q4" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!Q1" pad="3"/>
<connect gate="A" pin="!Q2" pad="6"/>
<connect gate="A" pin="!Q3" pad="11"/>
<connect gate="A" pin="!Q4" pad="14"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="5"/>
<connect gate="A" pin="D3" pad="12"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="10"/>
<connect gate="A" pin="Q4" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!Q1" pad="4"/>
<connect gate="A" pin="!Q2" pad="8"/>
<connect gate="A" pin="!Q3" pad="14"/>
<connect gate="A" pin="!Q4" pad="18"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="D1" pad="5"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="15"/>
<connect gate="A" pin="D4" pad="17"/>
<connect gate="A" pin="Q1" pad="3"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="13"/>
<connect gate="A" pin="Q4" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*176" prefix="IC">
<description>Presettable decade/binary &lt;b&gt;COUNTER/LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74176"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="4"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="CK1" pad="8"/>
<connect gate="A" pin="CK2" pad="6"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="D" pad="11"/>
<connect gate="A" pin="LD" pad="1"/>
<connect gate="A" pin="QA" pad="5"/>
<connect gate="A" pin="QB" pad="9"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*178" prefix="IC">
<description>4-bit parallel access &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74178"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="CLK" pad="5"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="LD" pad="9"/>
<connect gate="A" pin="QA" pad="4"/>
<connect gate="A" pin="QB" pad="6"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="10"/>
<connect gate="A" pin="SER" pad="3"/>
<connect gate="A" pin="SHF" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*179" prefix="IC">
<description>4-bit parallel access &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74179"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!QD" pad="12"/>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="CLK" pad="6"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="14"/>
<connect gate="A" pin="LD" pad="10"/>
<connect gate="A" pin="QA" pad="5"/>
<connect gate="A" pin="QB" pad="7"/>
<connect gate="A" pin="QC" pad="9"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="SER" pad="4"/>
<connect gate="A" pin="SHF" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*180" prefix="IC">
<description>9-bit odd/even &lt;B&gt;PARITY GENERATOR/CHECKER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74180"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="8"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="D" pad="11"/>
<connect gate="A" pin="E" pad="12"/>
<connect gate="A" pin="EI" pad="3"/>
<connect gate="A" pin="EVN" pad="5"/>
<connect gate="A" pin="F" pad="13"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="H" pad="2"/>
<connect gate="A" pin="ODD" pad="6"/>
<connect gate="A" pin="OI" pad="4"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*181" prefix="IC">
<description>&lt;b&gt;ARITHMETIC LOGIC UNIT&lt;/b&gt; function generator</description>
<gates>
<gate name="A" symbol="74181"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="A0" pad="2"/>
<connect gate="A" pin="A1" pad="23"/>
<connect gate="A" pin="A2" pad="21"/>
<connect gate="A" pin="A3" pad="19"/>
<connect gate="A" pin="A=B" pad="14"/>
<connect gate="A" pin="B0" pad="1"/>
<connect gate="A" pin="B1" pad="22"/>
<connect gate="A" pin="B2" pad="20"/>
<connect gate="A" pin="B3" pad="18"/>
<connect gate="A" pin="CN" pad="7"/>
<connect gate="A" pin="CN+4" pad="16"/>
<connect gate="A" pin="F0" pad="9"/>
<connect gate="A" pin="F1" pad="10"/>
<connect gate="A" pin="F2" pad="11"/>
<connect gate="A" pin="F3" pad="13"/>
<connect gate="A" pin="G" pad="17"/>
<connect gate="A" pin="M" pad="8"/>
<connect gate="A" pin="P" pad="15"/>
<connect gate="A" pin="S0" pad="6"/>
<connect gate="A" pin="S1" pad="5"/>
<connect gate="A" pin="S2" pad="4"/>
<connect gate="A" pin="S3" pad="3"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="DW" package="SO24W">
<connects>
<connect gate="A" pin="A0" pad="2"/>
<connect gate="A" pin="A1" pad="23"/>
<connect gate="A" pin="A2" pad="21"/>
<connect gate="A" pin="A3" pad="19"/>
<connect gate="A" pin="A=B" pad="14"/>
<connect gate="A" pin="B0" pad="1"/>
<connect gate="A" pin="B1" pad="22"/>
<connect gate="A" pin="B2" pad="20"/>
<connect gate="A" pin="B3" pad="18"/>
<connect gate="A" pin="CN" pad="7"/>
<connect gate="A" pin="CN+4" pad="16"/>
<connect gate="A" pin="F0" pad="9"/>
<connect gate="A" pin="F1" pad="10"/>
<connect gate="A" pin="F2" pad="11"/>
<connect gate="A" pin="F3" pad="13"/>
<connect gate="A" pin="G" pad="17"/>
<connect gate="A" pin="M" pad="8"/>
<connect gate="A" pin="P" pad="15"/>
<connect gate="A" pin="S0" pad="6"/>
<connect gate="A" pin="S1" pad="5"/>
<connect gate="A" pin="S2" pad="4"/>
<connect gate="A" pin="S3" pad="3"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC28">
<connects>
<connect gate="A" pin="A0" pad="3"/>
<connect gate="A" pin="A1" pad="27"/>
<connect gate="A" pin="A2" pad="25"/>
<connect gate="A" pin="A3" pad="23"/>
<connect gate="A" pin="A=B" pad="17"/>
<connect gate="A" pin="B0" pad="2"/>
<connect gate="A" pin="B1" pad="26"/>
<connect gate="A" pin="B2" pad="24"/>
<connect gate="A" pin="B3" pad="21"/>
<connect gate="A" pin="CN" pad="9"/>
<connect gate="A" pin="CN+4" pad="19"/>
<connect gate="A" pin="F0" pad="11"/>
<connect gate="A" pin="F1" pad="12"/>
<connect gate="A" pin="F2" pad="13"/>
<connect gate="A" pin="F3" pad="16"/>
<connect gate="A" pin="G" pad="20"/>
<connect gate="A" pin="M" pad="10"/>
<connect gate="A" pin="P" pad="18"/>
<connect gate="A" pin="S0" pad="7"/>
<connect gate="A" pin="S1" pad="6"/>
<connect gate="A" pin="S2" pad="5"/>
<connect gate="A" pin="S3" pad="4"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*182" prefix="IC">
<description>&lt;b&gt;LOOK AHEAD CARRY GENERATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74182"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CN" pad="13"/>
<connect gate="A" pin="CN+X" pad="12"/>
<connect gate="A" pin="CN+Y" pad="11"/>
<connect gate="A" pin="CN+Z" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="A" pin="G0" pad="3"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="14"/>
<connect gate="A" pin="G3" pad="5"/>
<connect gate="A" pin="P" pad="7"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="2"/>
<connect gate="A" pin="P2" pad="15"/>
<connect gate="A" pin="P3" pad="6"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="CN" pad="13"/>
<connect gate="A" pin="CN+X" pad="12"/>
<connect gate="A" pin="CN+Y" pad="11"/>
<connect gate="A" pin="CN+Z" pad="9"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="A" pin="G0" pad="3"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="14"/>
<connect gate="A" pin="G3" pad="5"/>
<connect gate="A" pin="P" pad="7"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="2"/>
<connect gate="A" pin="P2" pad="15"/>
<connect gate="A" pin="P3" pad="6"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="CN" pad="17"/>
<connect gate="A" pin="CN+X" pad="15"/>
<connect gate="A" pin="CN+Y" pad="14"/>
<connect gate="A" pin="CN+Z" pad="12"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="G0" pad="4"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="18"/>
<connect gate="A" pin="G3" pad="7"/>
<connect gate="A" pin="P" pad="9"/>
<connect gate="A" pin="P0" pad="5"/>
<connect gate="A" pin="P1" pad="3"/>
<connect gate="A" pin="P2" pad="19"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*183" prefix="IC">
<description>Dual carry save full &lt;b&gt;ADDER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74183"/>
<gate name="B" symbol="74183"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="CN" pad="4"/>
<connect gate="A" pin="CN+1" pad="5"/>
<connect gate="A" pin="S" pad="6"/>
<connect gate="B" pin="A" pad="13"/>
<connect gate="B" pin="B" pad="12"/>
<connect gate="B" pin="CN" pad="11"/>
<connect gate="B" pin="CN+1" pad="10"/>
<connect gate="B" pin="S" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="CN" pad="4"/>
<connect gate="A" pin="CN+1" pad="5"/>
<connect gate="A" pin="S" pad="6"/>
<connect gate="B" pin="A" pad="13"/>
<connect gate="B" pin="B" pad="12"/>
<connect gate="B" pin="CN" pad="11"/>
<connect gate="B" pin="CN+1" pad="10"/>
<connect gate="B" pin="S" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*184" prefix="IC">
<description>BCD to binary and binary to BCD &lt;b&gt;CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74184"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="11"/>
<connect gate="A" pin="C" pad="12"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="E" pad="14"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="2"/>
<connect gate="A" pin="Y3" pad="3"/>
<connect gate="A" pin="Y4" pad="4"/>
<connect gate="A" pin="Y5" pad="5"/>
<connect gate="A" pin="Y6" pad="6"/>
<connect gate="A" pin="Y7" pad="7"/>
<connect gate="A" pin="Y8" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*190" prefix="IC">
<description>Synchronous &lt;b&gt; UP/DOWN COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74190"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CTE" pad="4"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="D/!U" pad="5"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="MX/MN" pad="12"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
</technologies>
</device>
<device name="NS" package="SO16NS">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CTE" pad="4"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="D/!U" pad="5"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="MX/MN" pad="12"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
<device name="D" package="SO16D">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CTE" pad="4"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="D/!U" pad="5"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="MX/MN" pad="12"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
<device name="PW" package="SO16PW">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CTE" pad="4"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="D/!U" pad="5"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="MX/MN" pad="12"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*192" prefix="IC">
<description>Synchronous 4-bit &lt;b&gt;UP/DOWN COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74192"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="BO" pad="13"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="CO" pad="12"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="DN" pad="4"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="UP" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*194" prefix="IC">
<description>4-bit bidirectional &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74194"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="A" pin="S0" pad="9"/>
<connect gate="A" pin="S1" pad="10"/>
<connect gate="A" pin="SL" pad="7"/>
<connect gate="A" pin="SR" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="A" pin="S0" pad="9"/>
<connect gate="A" pin="S1" pad="10"/>
<connect gate="A" pin="SL" pad="7"/>
<connect gate="A" pin="SR" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="4"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="7"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="D" pad="8"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="18"/>
<connect gate="A" pin="QC" pad="17"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="S0" pad="12"/>
<connect gate="A" pin="S1" pad="13"/>
<connect gate="A" pin="SL" pad="9"/>
<connect gate="A" pin="SR" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*195" prefix="IC">
<description>4-bit parallel access &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74195"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!QD" pad="11"/>
<connect gate="A" pin="A" pad="4"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="6"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="J" pad="2"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="A" pin="S/!L" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!QD" pad="11"/>
<connect gate="A" pin="A" pad="4"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="6"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="7"/>
<connect gate="A" pin="J" pad="2"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="A" pin="S/!L" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!QD" pad="14"/>
<connect gate="A" pin="A" pad="5"/>
<connect gate="A" pin="B" pad="7"/>
<connect gate="A" pin="C" pad="8"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="J" pad="3"/>
<connect gate="A" pin="K" pad="4"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="18"/>
<connect gate="A" pin="QC" pad="17"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="S/!L" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*198" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74198"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="7"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="E" pad="15"/>
<connect gate="A" pin="F" pad="17"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="A" pin="H" pad="21"/>
<connect gate="A" pin="QA" pad="4"/>
<connect gate="A" pin="QB" pad="6"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="10"/>
<connect gate="A" pin="QE" pad="14"/>
<connect gate="A" pin="QF" pad="16"/>
<connect gate="A" pin="QG" pad="18"/>
<connect gate="A" pin="QH" pad="20"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="23"/>
<connect gate="A" pin="SL" pad="22"/>
<connect gate="A" pin="SR" pad="2"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*199" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74199"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="7"/>
<connect gate="A" pin="CINH" pad="11"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="E" pad="16"/>
<connect gate="A" pin="F" pad="18"/>
<connect gate="A" pin="G" pad="20"/>
<connect gate="A" pin="H" pad="22"/>
<connect gate="A" pin="J" pad="2"/>
<connect gate="A" pin="K" pad="1"/>
<connect gate="A" pin="QA" pad="4"/>
<connect gate="A" pin="QB" pad="6"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="10"/>
<connect gate="A" pin="QE" pad="15"/>
<connect gate="A" pin="QF" pad="17"/>
<connect gate="A" pin="QG" pad="19"/>
<connect gate="A" pin="QH" pad="21"/>
<connect gate="A" pin="SH/!LD" pad="23"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*240" prefix="IC">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74240"/>
<gate name="B" symbol="74240"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*241" prefix="IC">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74241"/>
<gate name="P" symbol="PWRN"/>
<gate name="B" symbol="74241A"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*242" prefix="IC">
<description>Quadruple &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74242"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="10"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="B4" pad="8"/>
<connect gate="A" pin="GAB" pad="1"/>
<connect gate="A" pin="GBA" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*244" prefix="IC">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74244"/>
<gate name="B" symbol="74244"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*245" prefix="IC">
<description>Octal &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74245"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="DIR" pad="1"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*250" prefix="IC">
<description>1 of 16 data &lt;b&gt;GENERATOR/MULTIPLEXER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74250"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="11"/>
<connect gate="A" pin="E0" pad="8"/>
<connect gate="A" pin="E1" pad="7"/>
<connect gate="A" pin="E10" pad="21"/>
<connect gate="A" pin="E11" pad="20"/>
<connect gate="A" pin="E12" pad="19"/>
<connect gate="A" pin="E13" pad="18"/>
<connect gate="A" pin="E14" pad="17"/>
<connect gate="A" pin="E15" pad="16"/>
<connect gate="A" pin="E2" pad="6"/>
<connect gate="A" pin="E3" pad="5"/>
<connect gate="A" pin="E4" pad="4"/>
<connect gate="A" pin="E5" pad="3"/>
<connect gate="A" pin="E6" pad="2"/>
<connect gate="A" pin="E7" pad="1"/>
<connect gate="A" pin="E8" pad="23"/>
<connect gate="A" pin="E9" pad="22"/>
<connect gate="A" pin="G" pad="9"/>
<connect gate="A" pin="W" pad="10"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*251" prefix="IC">
<description>1 of 8 data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74251"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="D0" pad="4"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="2"/>
<connect gate="A" pin="D3" pad="1"/>
<connect gate="A" pin="D4" pad="15"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="13"/>
<connect gate="A" pin="D7" pad="12"/>
<connect gate="A" pin="G" pad="7"/>
<connect gate="A" pin="W" pad="6"/>
<connect gate="A" pin="Y" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="11"/>
<connect gate="A" pin="B" pad="10"/>
<connect gate="A" pin="C" pad="9"/>
<connect gate="A" pin="D0" pad="4"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="2"/>
<connect gate="A" pin="D3" pad="1"/>
<connect gate="A" pin="D4" pad="15"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="13"/>
<connect gate="A" pin="D7" pad="12"/>
<connect gate="A" pin="G" pad="7"/>
<connect gate="A" pin="W" pad="6"/>
<connect gate="A" pin="Y" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="13"/>
<connect gate="A" pin="C" pad="12"/>
<connect gate="A" pin="D0" pad="5"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="19"/>
<connect gate="A" pin="D5" pad="18"/>
<connect gate="A" pin="D6" pad="17"/>
<connect gate="A" pin="D7" pad="15"/>
<connect gate="A" pin="G" pad="9"/>
<connect gate="A" pin="W" pad="8"/>
<connect gate="A" pin="Y" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*253" prefix="IC">
<description>Dual 4-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74253"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1C0" pad="6"/>
<connect gate="A" pin="1C1" pad="5"/>
<connect gate="A" pin="1C2" pad="4"/>
<connect gate="A" pin="1C3" pad="3"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y" pad="7"/>
<connect gate="A" pin="2C0" pad="10"/>
<connect gate="A" pin="2C1" pad="11"/>
<connect gate="A" pin="2C2" pad="12"/>
<connect gate="A" pin="2C3" pad="13"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C0" pad="6"/>
<connect gate="A" pin="1C1" pad="5"/>
<connect gate="A" pin="1C2" pad="4"/>
<connect gate="A" pin="1C3" pad="3"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y" pad="7"/>
<connect gate="A" pin="2C0" pad="10"/>
<connect gate="A" pin="2C1" pad="11"/>
<connect gate="A" pin="2C2" pad="12"/>
<connect gate="A" pin="2C3" pad="13"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1C0" pad="8"/>
<connect gate="A" pin="1C1" pad="7"/>
<connect gate="A" pin="1C2" pad="5"/>
<connect gate="A" pin="1C3" pad="4"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y" pad="9"/>
<connect gate="A" pin="2C0" pad="13"/>
<connect gate="A" pin="2C1" pad="14"/>
<connect gate="A" pin="2C2" pad="15"/>
<connect gate="A" pin="2C3" pad="17"/>
<connect gate="A" pin="2G" pad="19"/>
<connect gate="A" pin="2Y" pad="12"/>
<connect gate="A" pin="A" pad="18"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*257" prefix="IC">
<description>Quadruple 2-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74257"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!A!/B" pad="2"/>
<connect gate="A" pin="1A" pad="3"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1Y" pad="5"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="4A" pad="18"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4Y" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*258" prefix="IC">
<description>Quadruple 2-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74258"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!A!/B" pad="1"/>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="11"/>
<connect gate="A" pin="3B" pad="10"/>
<connect gate="A" pin="3Y" pad="9"/>
<connect gate="A" pin="4A" pad="14"/>
<connect gate="A" pin="4B" pad="13"/>
<connect gate="A" pin="4Y" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!A!/B" pad="2"/>
<connect gate="A" pin="1A" pad="3"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1Y" pad="5"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="3A" pad="14"/>
<connect gate="A" pin="3B" pad="13"/>
<connect gate="A" pin="3Y" pad="12"/>
<connect gate="A" pin="4A" pad="18"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4Y" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*259" prefix="IC">
<description>8-bit addressable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74259"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CLR" pad="15"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="Q0" pad="4"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="CLR" pad="15"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="Q0" pad="4"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="6"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="10"/>
<connect gate="A" pin="Q6" pad="11"/>
<connect gate="A" pin="Q7" pad="12"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*261" prefix="IC">
<description>2 by 4 bit parallel binary &lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74261"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="B0" pad="13"/>
<connect gate="A" pin="B1" pad="14"/>
<connect gate="A" pin="B2" pad="15"/>
<connect gate="A" pin="B3" pad="1"/>
<connect gate="A" pin="B4" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="M0" pad="11"/>
<connect gate="A" pin="M1" pad="12"/>
<connect gate="A" pin="M2" pad="4"/>
<connect gate="A" pin="Q0" pad="10"/>
<connect gate="A" pin="Q1" pad="9"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="5"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*273" prefix="IC">
<description>Octal D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="A" symbol="74273"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="7"/>
<connect gate="A" pin="D4" pad="8"/>
<connect gate="A" pin="D5" pad="13"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="17"/>
<connect gate="A" pin="D8" pad="18"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="12"/>
<connect gate="A" pin="Q6" pad="15"/>
<connect gate="A" pin="Q7" pad="16"/>
<connect gate="A" pin="Q8" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="7"/>
<connect gate="A" pin="D4" pad="8"/>
<connect gate="A" pin="D5" pad="13"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="17"/>
<connect gate="A" pin="D8" pad="18"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="12"/>
<connect gate="A" pin="Q6" pad="15"/>
<connect gate="A" pin="Q7" pad="16"/>
<connect gate="A" pin="Q8" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="7"/>
<connect gate="A" pin="D4" pad="8"/>
<connect gate="A" pin="D5" pad="13"/>
<connect gate="A" pin="D6" pad="14"/>
<connect gate="A" pin="D7" pad="17"/>
<connect gate="A" pin="D8" pad="18"/>
<connect gate="A" pin="Q1" pad="2"/>
<connect gate="A" pin="Q2" pad="5"/>
<connect gate="A" pin="Q3" pad="6"/>
<connect gate="A" pin="Q4" pad="9"/>
<connect gate="A" pin="Q5" pad="12"/>
<connect gate="A" pin="Q6" pad="15"/>
<connect gate="A" pin="Q7" pad="16"/>
<connect gate="A" pin="Q8" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*276" prefix="IC">
<description>Quadruple J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74276"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1CK" pad="3"/>
<connect gate="A" pin="1J" pad="2"/>
<connect gate="A" pin="1K" pad="4"/>
<connect gate="A" pin="1Q" pad="5"/>
<connect gate="A" pin="2CK" pad="8"/>
<connect gate="A" pin="2J" pad="9"/>
<connect gate="A" pin="2K" pad="7"/>
<connect gate="A" pin="2Q" pad="6"/>
<connect gate="A" pin="3CK" pad="13"/>
<connect gate="A" pin="3J" pad="12"/>
<connect gate="A" pin="3K" pad="14"/>
<connect gate="A" pin="3Q" pad="15"/>
<connect gate="A" pin="4CK" pad="18"/>
<connect gate="A" pin="4J" pad="19"/>
<connect gate="A" pin="4K" pad="17"/>
<connect gate="A" pin="4Q" pad="16"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="PRE" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*278" prefix="IC">
<description>4-bit cascadable &lt;b&gt;PRIORITY REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74278"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="D1" pad="12"/>
<connect gate="A" pin="D2" pad="13"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="3"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="5"/>
<connect gate="A" pin="STR" pad="1"/>
<connect gate="A" pin="Y1" pad="10"/>
<connect gate="A" pin="Y2" pad="9"/>
<connect gate="A" pin="Y3" pad="8"/>
<connect gate="A" pin="Y4" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*279" prefix="IC">
<description>Quadruple S-R &lt;B&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74279A"/>
<gate name="B" symbol="74279A"/>
<gate name="C" symbol="74279B"/>
<gate name="D" symbol="74279B"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="Q" pad="4"/>
<connect gate="A" pin="R" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="B" pin="R" pad="10"/>
<connect gate="B" pin="S1" pad="11"/>
<connect gate="B" pin="S2" pad="12"/>
<connect gate="C" pin="Q" pad="7"/>
<connect gate="C" pin="R" pad="5"/>
<connect gate="C" pin="S" pad="6"/>
<connect gate="D" pin="Q" pad="13"/>
<connect gate="D" pin="R" pad="14"/>
<connect gate="D" pin="S" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="Q" pad="4"/>
<connect gate="A" pin="R" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="B" pin="R" pad="10"/>
<connect gate="B" pin="S1" pad="11"/>
<connect gate="B" pin="S2" pad="12"/>
<connect gate="C" pin="Q" pad="7"/>
<connect gate="C" pin="R" pad="5"/>
<connect gate="C" pin="S" pad="6"/>
<connect gate="D" pin="Q" pad="13"/>
<connect gate="D" pin="R" pad="14"/>
<connect gate="D" pin="S" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="A" pin="R" pad="2"/>
<connect gate="A" pin="S1" pad="3"/>
<connect gate="A" pin="S2" pad="4"/>
<connect gate="B" pin="Q" pad="12"/>
<connect gate="B" pin="R" pad="13"/>
<connect gate="B" pin="S1" pad="14"/>
<connect gate="B" pin="S2" pad="15"/>
<connect gate="C" pin="Q" pad="9"/>
<connect gate="C" pin="R" pad="7"/>
<connect gate="C" pin="S" pad="8"/>
<connect gate="D" pin="Q" pad="17"/>
<connect gate="D" pin="R" pad="18"/>
<connect gate="D" pin="S" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*280" prefix="IC">
<description>9-bit odd/even &lt;b&gt;PARITY GENERATOR/CHECKER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74280"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="8"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="D" pad="11"/>
<connect gate="A" pin="E" pad="12"/>
<connect gate="A" pin="F" pad="13"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="H" pad="2"/>
<connect gate="A" pin="I" pad="4"/>
<connect gate="A" pin="SEV" pad="5"/>
<connect gate="A" pin="SOD" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="A" pad="8"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="D" pad="11"/>
<connect gate="A" pin="E" pad="12"/>
<connect gate="A" pin="F" pad="13"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="H" pad="2"/>
<connect gate="A" pin="I" pad="4"/>
<connect gate="A" pin="SEV" pad="5"/>
<connect gate="A" pin="SOD" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="12"/>
<connect gate="A" pin="B" pad="13"/>
<connect gate="A" pin="C" pad="14"/>
<connect gate="A" pin="D" pad="16"/>
<connect gate="A" pin="E" pad="18"/>
<connect gate="A" pin="F" pad="19"/>
<connect gate="A" pin="G" pad="2"/>
<connect gate="A" pin="H" pad="3"/>
<connect gate="A" pin="I" pad="6"/>
<connect gate="A" pin="SEV" pad="8"/>
<connect gate="A" pin="SOD" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*283" prefix="IC">
<description>4-bit binary &lt;b&gt;FULL ADDER&lt;/b&gt;, fast carry</description>
<gates>
<gate name="A" symbol="74283"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="5"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="6"/>
<connect gate="A" pin="B2" pad="2"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="11"/>
<connect gate="A" pin="C0" pad="7"/>
<connect gate="A" pin="C4" pad="9"/>
<connect gate="A" pin="S1" pad="4"/>
<connect gate="A" pin="S2" pad="1"/>
<connect gate="A" pin="S3" pad="13"/>
<connect gate="A" pin="S4" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A1" pad="5"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="12"/>
<connect gate="A" pin="B1" pad="6"/>
<connect gate="A" pin="B2" pad="2"/>
<connect gate="A" pin="B3" pad="15"/>
<connect gate="A" pin="B4" pad="11"/>
<connect gate="A" pin="C0" pad="7"/>
<connect gate="A" pin="C4" pad="9"/>
<connect gate="A" pin="S1" pad="4"/>
<connect gate="A" pin="S2" pad="1"/>
<connect gate="A" pin="S3" pad="13"/>
<connect gate="A" pin="S4" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="18"/>
<connect gate="A" pin="A4" pad="15"/>
<connect gate="A" pin="B1" pad="8"/>
<connect gate="A" pin="B2" pad="3"/>
<connect gate="A" pin="B3" pad="19"/>
<connect gate="A" pin="B4" pad="14"/>
<connect gate="A" pin="C0" pad="9"/>
<connect gate="A" pin="C4" pad="12"/>
<connect gate="A" pin="S1" pad="5"/>
<connect gate="A" pin="S2" pad="2"/>
<connect gate="A" pin="S3" pad="17"/>
<connect gate="A" pin="S4" pad="13"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*284" prefix="IC">
<description>4 by 4 parallel &lt;b&gt;BINARY MULTIPLIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74284"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1A" pad="5"/>
<connect gate="A" pin="1B" pad="6"/>
<connect gate="A" pin="1C" pad="7"/>
<connect gate="A" pin="1D" pad="4"/>
<connect gate="A" pin="2A" pad="3"/>
<connect gate="A" pin="2B" pad="2"/>
<connect gate="A" pin="2C" pad="1"/>
<connect gate="A" pin="2D" pad="15"/>
<connect gate="A" pin="GA" pad="14"/>
<connect gate="A" pin="GB" pad="13"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="10"/>
<connect gate="A" pin="Y7" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*285" prefix="IC">
<description>4 by 4 parallel &lt;b&gt;BINARY MULTIPLIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74285"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1A" pad="5"/>
<connect gate="A" pin="1B" pad="6"/>
<connect gate="A" pin="1C" pad="7"/>
<connect gate="A" pin="1D" pad="4"/>
<connect gate="A" pin="2A" pad="3"/>
<connect gate="A" pin="2B" pad="2"/>
<connect gate="A" pin="2C" pad="1"/>
<connect gate="A" pin="2D" pad="15"/>
<connect gate="A" pin="GA" pad="14"/>
<connect gate="A" pin="GB" pad="13"/>
<connect gate="A" pin="Y0" pad="12"/>
<connect gate="A" pin="Y1" pad="11"/>
<connect gate="A" pin="Y2" pad="10"/>
<connect gate="A" pin="Y3" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*286" prefix="IC">
<description>9-bit &lt;b&gt;PARITY GENERATOR/CHECKER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74286"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="8"/>
<connect gate="A" pin="B" pad="9"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="D" pad="11"/>
<connect gate="A" pin="E" pad="12"/>
<connect gate="A" pin="F" pad="13"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="H" pad="2"/>
<connect gate="A" pin="I" pad="4"/>
<connect gate="A" pin="PAR_ERR" pad="5"/>
<connect gate="A" pin="PAR_I/O" pad="6"/>
<connect gate="A" pin="XMIT" pad="3"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*290" prefix="IC">
<description>Decade and 4-bit &lt;b&gt;BINARY COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74290"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="11"/>
<connect gate="A" pin="QA" pad="9"/>
<connect gate="A" pin="QB" pad="5"/>
<connect gate="A" pin="QC" pad="4"/>
<connect gate="A" pin="QD" pad="8"/>
<connect gate="A" pin="R0(1)" pad="12"/>
<connect gate="A" pin="R0(2)" pad="13"/>
<connect gate="A" pin="R9(1)" pad="1"/>
<connect gate="A" pin="R9(2)" pad="3"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*292" prefix="IC">
<description>Programmable frequency &lt;b&gt;DIVIDER/DIGITAL TIMER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74292"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="CK1" pad="4"/>
<connect gate="A" pin="CK2" pad="5"/>
<connect gate="A" pin="CLR" pad="11"/>
<connect gate="A" pin="D" pad="14"/>
<connect gate="A" pin="E" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="TP1" pad="3"/>
<connect gate="A" pin="TP2" pad="6"/>
<connect gate="A" pin="TP3" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="13"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="19"/>
<connect gate="A" pin="CK1" pad="5"/>
<connect gate="A" pin="CK2" pad="7"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D" pad="18"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="A" pin="Q" pad="9"/>
<connect gate="A" pin="TP1" pad="4"/>
<connect gate="A" pin="TP2" pad="8"/>
<connect gate="A" pin="TP3" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*293" prefix="IC">
<description>Decade and 4-bit &lt;b&gt;BINARY COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74293"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="11"/>
<connect gate="A" pin="QA" pad="9"/>
<connect gate="A" pin="QB" pad="5"/>
<connect gate="A" pin="QC" pad="4"/>
<connect gate="A" pin="QD" pad="8"/>
<connect gate="A" pin="R0(1)" pad="12"/>
<connect gate="A" pin="R0(2)" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="A" pad="10"/>
<connect gate="A" pin="B" pad="11"/>
<connect gate="A" pin="QA" pad="9"/>
<connect gate="A" pin="QB" pad="5"/>
<connect gate="A" pin="QC" pad="4"/>
<connect gate="A" pin="QD" pad="8"/>
<connect gate="A" pin="R0(1)" pad="12"/>
<connect gate="A" pin="R0(2)" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*294" prefix="IC">
<description>Programmable frequency &lt;b&gt;DIVIDER/DIGITAL TIMER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74294"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="CK1" pad="4"/>
<connect gate="A" pin="CK2" pad="5"/>
<connect gate="A" pin="CLR" pad="11"/>
<connect gate="A" pin="D" pad="14"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="A" pin="TP" pad="3"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="19"/>
<connect gate="A" pin="CK1" pad="5"/>
<connect gate="A" pin="CK2" pad="7"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="D" pad="18"/>
<connect gate="A" pin="Q" pad="9"/>
<connect gate="A" pin="TP" pad="4"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*295" prefix="IC">
<description>4-bit right/left &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74295"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="3"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="D" pad="5"/>
<connect gate="A" pin="LD/!SH" pad="6"/>
<connect gate="A" pin="OC" pad="8"/>
<connect gate="A" pin="QA" pad="13"/>
<connect gate="A" pin="QB" pad="12"/>
<connect gate="A" pin="QC" pad="11"/>
<connect gate="A" pin="QD" pad="10"/>
<connect gate="A" pin="SER" pad="1"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*298" prefix="IC">
<description>Quadruple 2-input &lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74298"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="B1" pad="4"/>
<connect gate="A" pin="B2" pad="1"/>
<connect gate="A" pin="C1" pad="9"/>
<connect gate="A" pin="C2" pad="5"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="A" pin="WS" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="B1" pad="4"/>
<connect gate="A" pin="B2" pad="1"/>
<connect gate="A" pin="C1" pad="9"/>
<connect gate="A" pin="C2" pad="5"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="A" pin="WS" pad="10"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="2"/>
<connect gate="A" pin="C1" pad="12"/>
<connect gate="A" pin="C2" pad="7"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="D1" pad="9"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="18"/>
<connect gate="A" pin="QC" pad="17"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="WS" pad="13"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*299" prefix="IC">
<description>8-bit universal &lt;b&gt;SHIFT/STORAGE REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74299"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A/QA" pad="7"/>
<connect gate="A" pin="B/QB" pad="13"/>
<connect gate="A" pin="C/QC" pad="6"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="D/QD" pad="14"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="15"/>
<connect gate="A" pin="G/QG" pad="4"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="3"/>
<connect gate="A" pin="H/QH" pad="16"/>
<connect gate="A" pin="QA*" pad="8"/>
<connect gate="A" pin="QH*" pad="17"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="19"/>
<connect gate="A" pin="SL" pad="18"/>
<connect gate="A" pin="SR" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A/QA" pad="7"/>
<connect gate="A" pin="B/QB" pad="13"/>
<connect gate="A" pin="C/QC" pad="6"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="D/QD" pad="14"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="15"/>
<connect gate="A" pin="G/QG" pad="4"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="3"/>
<connect gate="A" pin="H/QH" pad="16"/>
<connect gate="A" pin="QA*" pad="8"/>
<connect gate="A" pin="QH*" pad="17"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="19"/>
<connect gate="A" pin="SL" pad="18"/>
<connect gate="A" pin="SR" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A/QA" pad="7"/>
<connect gate="A" pin="B/QB" pad="13"/>
<connect gate="A" pin="C/QC" pad="6"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="D/QD" pad="14"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="15"/>
<connect gate="A" pin="G/QG" pad="4"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="3"/>
<connect gate="A" pin="H/QH" pad="16"/>
<connect gate="A" pin="QA*" pad="8"/>
<connect gate="A" pin="QH*" pad="17"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="19"/>
<connect gate="A" pin="SL" pad="18"/>
<connect gate="A" pin="SR" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*320" prefix="IC">
<description>Crystal controlled &lt;b&gt;OSCILLATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74320"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!F" pad="12"/>
<connect gate="A" pin="!F*" pad="9"/>
<connect gate="A" pin="F" pad="7"/>
<connect gate="A" pin="F*" pad="10"/>
<connect gate="A" pin="FFD" pad="5"/>
<connect gate="A" pin="FFQ" pad="4"/>
<connect gate="A" pin="TK1" pad="1"/>
<connect gate="A" pin="TK2" pad="2"/>
<connect gate="A" pin="XTL@1" pad="14"/>
<connect gate="A" pin="XTL@2" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*321" prefix="IC">
<description>Crystal controlled &lt;b&gt;OSCILLATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74321"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!F" pad="12"/>
<connect gate="A" pin="!F*" pad="9"/>
<connect gate="A" pin="F" pad="7"/>
<connect gate="A" pin="F*" pad="10"/>
<connect gate="A" pin="F/2" pad="13"/>
<connect gate="A" pin="F/4" pad="6"/>
<connect gate="A" pin="FFD" pad="5"/>
<connect gate="A" pin="FFQ" pad="4"/>
<connect gate="A" pin="TK1" pad="1"/>
<connect gate="A" pin="TK2" pad="2"/>
<connect gate="A" pin="XTL@1" pad="14"/>
<connect gate="A" pin="XTL@2" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*322" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74322"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A/QA" pad="4"/>
<connect gate="A" pin="B/QB" pad="16"/>
<connect gate="A" pin="C/QC" pad="5"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="CLR" pad="9"/>
<connect gate="A" pin="D/QD" pad="15"/>
<connect gate="A" pin="D0" pad="3"/>
<connect gate="A" pin="D1" pad="17"/>
<connect gate="A" pin="DS" pad="19"/>
<connect gate="A" pin="E/QE" pad="6"/>
<connect gate="A" pin="F/QF" pad="14"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="G/QG" pad="7"/>
<connect gate="A" pin="H/QH" pad="13"/>
<connect gate="A" pin="OE" pad="8"/>
<connect gate="A" pin="QH*" pad="12"/>
<connect gate="A" pin="S/!P" pad="2"/>
<connect gate="A" pin="SE" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*348" prefix="IC">
<description>8-to 3 line &lt;b&gt;PRIORITY ENCODER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74348"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="0" pad="10"/>
<connect gate="A" pin="1" pad="11"/>
<connect gate="A" pin="2" pad="12"/>
<connect gate="A" pin="3" pad="13"/>
<connect gate="A" pin="4" pad="1"/>
<connect gate="A" pin="5" pad="2"/>
<connect gate="A" pin="6" pad="3"/>
<connect gate="A" pin="7" pad="4"/>
<connect gate="A" pin="A0" pad="9"/>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A2" pad="6"/>
<connect gate="A" pin="E0" pad="15"/>
<connect gate="A" pin="EI" pad="5"/>
<connect gate="A" pin="GS" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="0" pad="10"/>
<connect gate="A" pin="1" pad="11"/>
<connect gate="A" pin="2" pad="12"/>
<connect gate="A" pin="3" pad="13"/>
<connect gate="A" pin="4" pad="1"/>
<connect gate="A" pin="5" pad="2"/>
<connect gate="A" pin="6" pad="3"/>
<connect gate="A" pin="7" pad="4"/>
<connect gate="A" pin="A0" pad="9"/>
<connect gate="A" pin="A1" pad="7"/>
<connect gate="A" pin="A2" pad="6"/>
<connect gate="A" pin="E0" pad="15"/>
<connect gate="A" pin="EI" pad="5"/>
<connect gate="A" pin="GS" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="0" pad="13"/>
<connect gate="A" pin="1" pad="14"/>
<connect gate="A" pin="2" pad="15"/>
<connect gate="A" pin="3" pad="17"/>
<connect gate="A" pin="4" pad="2"/>
<connect gate="A" pin="5" pad="3"/>
<connect gate="A" pin="6" pad="4"/>
<connect gate="A" pin="7" pad="5"/>
<connect gate="A" pin="A0" pad="12"/>
<connect gate="A" pin="A1" pad="9"/>
<connect gate="A" pin="A2" pad="8"/>
<connect gate="A" pin="E0" pad="19"/>
<connect gate="A" pin="EI" pad="7"/>
<connect gate="A" pin="GS" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*352" prefix="IC">
<description>Dual 4-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74352"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1C0" pad="6"/>
<connect gate="A" pin="1C1" pad="5"/>
<connect gate="A" pin="1C2" pad="4"/>
<connect gate="A" pin="1C3" pad="3"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y" pad="7"/>
<connect gate="A" pin="2C0" pad="10"/>
<connect gate="A" pin="2C1" pad="11"/>
<connect gate="A" pin="2C2" pad="12"/>
<connect gate="A" pin="2C3" pad="13"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1C0" pad="6"/>
<connect gate="A" pin="1C1" pad="5"/>
<connect gate="A" pin="1C2" pad="4"/>
<connect gate="A" pin="1C3" pad="3"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y" pad="7"/>
<connect gate="A" pin="2C0" pad="10"/>
<connect gate="A" pin="2C1" pad="11"/>
<connect gate="A" pin="2C2" pad="12"/>
<connect gate="A" pin="2C3" pad="13"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*353" prefix="IC">
<description>Dual 4-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74353"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1C0" pad="6"/>
<connect gate="A" pin="1C1" pad="5"/>
<connect gate="A" pin="1C2" pad="4"/>
<connect gate="A" pin="1C3" pad="3"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y" pad="7"/>
<connect gate="A" pin="2C0" pad="10"/>
<connect gate="A" pin="2C1" pad="11"/>
<connect gate="A" pin="2C2" pad="12"/>
<connect gate="A" pin="2C3" pad="13"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*354" prefix="IC">
<description>8-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER/REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74354"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="D0" pad="8"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="D5" pad="3"/>
<connect gate="A" pin="D6" pad="2"/>
<connect gate="A" pin="D7" pad="1"/>
<connect gate="A" pin="DC" pad="9"/>
<connect gate="A" pin="G1" pad="15"/>
<connect gate="A" pin="G2" pad="16"/>
<connect gate="A" pin="G3" pad="17"/>
<connect gate="A" pin="S0" pad="14"/>
<connect gate="A" pin="S1" pad="13"/>
<connect gate="A" pin="S2" pad="12"/>
<connect gate="A" pin="SC" pad="11"/>
<connect gate="A" pin="W" pad="18"/>
<connect gate="A" pin="Y" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*355" prefix="IC">
<description>8-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER/REGISTER&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="74355"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="D0" pad="8"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="D5" pad="3"/>
<connect gate="A" pin="D6" pad="2"/>
<connect gate="A" pin="D7" pad="1"/>
<connect gate="A" pin="DC" pad="9"/>
<connect gate="A" pin="G1" pad="15"/>
<connect gate="A" pin="G2" pad="16"/>
<connect gate="A" pin="G3" pad="17"/>
<connect gate="A" pin="S0" pad="14"/>
<connect gate="A" pin="S1" pad="13"/>
<connect gate="A" pin="S2" pad="12"/>
<connect gate="A" pin="SC" pad="11"/>
<connect gate="A" pin="W" pad="18"/>
<connect gate="A" pin="Y" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*356" prefix="IC">
<description>8-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER/REGISTER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74356"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="D0" pad="8"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="D5" pad="3"/>
<connect gate="A" pin="D6" pad="2"/>
<connect gate="A" pin="D7" pad="1"/>
<connect gate="A" pin="G1" pad="15"/>
<connect gate="A" pin="G2" pad="16"/>
<connect gate="A" pin="G3" pad="17"/>
<connect gate="A" pin="S0" pad="14"/>
<connect gate="A" pin="S1" pad="13"/>
<connect gate="A" pin="S2" pad="12"/>
<connect gate="A" pin="SC" pad="11"/>
<connect gate="A" pin="W" pad="18"/>
<connect gate="A" pin="Y" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*357" prefix="IC">
<description>8-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER/REGISTER&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="74357"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="D0" pad="8"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="D5" pad="3"/>
<connect gate="A" pin="D6" pad="2"/>
<connect gate="A" pin="D7" pad="1"/>
<connect gate="A" pin="G1" pad="15"/>
<connect gate="A" pin="G2" pad="16"/>
<connect gate="A" pin="G3" pad="17"/>
<connect gate="A" pin="S0" pad="14"/>
<connect gate="A" pin="S1" pad="13"/>
<connect gate="A" pin="S2" pad="12"/>
<connect gate="A" pin="SC" pad="11"/>
<connect gate="A" pin="W" pad="18"/>
<connect gate="A" pin="Y" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*365" prefix="IC">
<description>Hex &lt;b&gt;BUS DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74365"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="10"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="15"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="10"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="15"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="8"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="A5" pad="15"/>
<connect gate="A" pin="A6" pad="18"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="4"/>
<connect gate="A" pin="Y2" pad="7"/>
<connect gate="A" pin="Y3" pad="9"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*366" prefix="IC">
<description>Hex &lt;b&gt;BUS DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74366"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="10"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="15"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="10"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="15"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="8"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="A5" pad="15"/>
<connect gate="A" pin="A6" pad="18"/>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="4"/>
<connect gate="A" pin="Y2" pad="7"/>
<connect gate="A" pin="Y3" pad="9"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*367" prefix="IC">
<description>Hex &lt;b&gt;BUS DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74367"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1A1" pad="2"/>
<connect gate="A" pin="1A2" pad="4"/>
<connect gate="A" pin="1A3" pad="6"/>
<connect gate="A" pin="1A4" pad="10"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y1" pad="3"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="7"/>
<connect gate="A" pin="1Y4" pad="9"/>
<connect gate="A" pin="2A1" pad="12"/>
<connect gate="A" pin="2A2" pad="14"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y1" pad="11"/>
<connect gate="A" pin="2Y2" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1A1" pad="2"/>
<connect gate="A" pin="1A2" pad="4"/>
<connect gate="A" pin="1A3" pad="6"/>
<connect gate="A" pin="1A4" pad="10"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y1" pad="3"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="7"/>
<connect gate="A" pin="1Y4" pad="9"/>
<connect gate="A" pin="2A1" pad="12"/>
<connect gate="A" pin="2A2" pad="14"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y1" pad="11"/>
<connect gate="A" pin="2Y2" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1A1" pad="3"/>
<connect gate="A" pin="1A2" pad="5"/>
<connect gate="A" pin="1A3" pad="8"/>
<connect gate="A" pin="1A4" pad="13"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y1" pad="4"/>
<connect gate="A" pin="1Y2" pad="7"/>
<connect gate="A" pin="1Y3" pad="9"/>
<connect gate="A" pin="1Y4" pad="12"/>
<connect gate="A" pin="2A1" pad="15"/>
<connect gate="A" pin="2A2" pad="18"/>
<connect gate="A" pin="2G" pad="19"/>
<connect gate="A" pin="2Y1" pad="14"/>
<connect gate="A" pin="2Y2" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*368" prefix="IC">
<description>Hex &lt;b&gt;BUS DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74368"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1A1" pad="2"/>
<connect gate="A" pin="1A2" pad="4"/>
<connect gate="A" pin="1A3" pad="6"/>
<connect gate="A" pin="1A4" pad="10"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y1" pad="3"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="7"/>
<connect gate="A" pin="1Y4" pad="9"/>
<connect gate="A" pin="2A1" pad="12"/>
<connect gate="A" pin="2A2" pad="14"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y1" pad="11"/>
<connect gate="A" pin="2Y2" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1A1" pad="2"/>
<connect gate="A" pin="1A2" pad="4"/>
<connect gate="A" pin="1A3" pad="6"/>
<connect gate="A" pin="1A4" pad="10"/>
<connect gate="A" pin="1G" pad="1"/>
<connect gate="A" pin="1Y1" pad="3"/>
<connect gate="A" pin="1Y2" pad="5"/>
<connect gate="A" pin="1Y3" pad="7"/>
<connect gate="A" pin="1Y4" pad="9"/>
<connect gate="A" pin="2A1" pad="12"/>
<connect gate="A" pin="2A2" pad="14"/>
<connect gate="A" pin="2G" pad="15"/>
<connect gate="A" pin="2Y1" pad="11"/>
<connect gate="A" pin="2Y2" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1A1" pad="3"/>
<connect gate="A" pin="1A2" pad="5"/>
<connect gate="A" pin="1A3" pad="8"/>
<connect gate="A" pin="1A4" pad="13"/>
<connect gate="A" pin="1G" pad="2"/>
<connect gate="A" pin="1Y1" pad="4"/>
<connect gate="A" pin="1Y2" pad="7"/>
<connect gate="A" pin="1Y3" pad="9"/>
<connect gate="A" pin="1Y4" pad="12"/>
<connect gate="A" pin="2A1" pad="15"/>
<connect gate="A" pin="2A2" pad="18"/>
<connect gate="A" pin="2G" pad="19"/>
<connect gate="A" pin="2Y1" pad="14"/>
<connect gate="A" pin="2Y2" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*373" prefix="IC">
<description>Octal D type transparent &lt;b&gt;LATCH&lt;/b&gt;, edge triggered</description>
<gates>
<gate name="A" symbol="74373"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="ENC" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="ENC" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="ENC" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*374" prefix="IC">
<description>Octal D type transparent &lt;b&gt;LATCH&lt;/b&gt;, edge triggered</description>
<gates>
<gate name="A" symbol="74374"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*375" prefix="IC">
<description>4-bit bistable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74375"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!1Q" pad="2"/>
<connect gate="A" pin="!2Q" pad="6"/>
<connect gate="A" pin="!3Q" pad="10"/>
<connect gate="A" pin="!4Q" pad="14"/>
<connect gate="A" pin="12C" pad="4"/>
<connect gate="A" pin="1D" pad="1"/>
<connect gate="A" pin="1Q" pad="3"/>
<connect gate="A" pin="2D" pad="7"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="34C" pad="12"/>
<connect gate="A" pin="3D" pad="9"/>
<connect gate="A" pin="3Q" pad="11"/>
<connect gate="A" pin="4D" pad="15"/>
<connect gate="A" pin="4Q" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!1Q" pad="2"/>
<connect gate="A" pin="!2Q" pad="6"/>
<connect gate="A" pin="!3Q" pad="10"/>
<connect gate="A" pin="!4Q" pad="14"/>
<connect gate="A" pin="12C" pad="4"/>
<connect gate="A" pin="1D" pad="1"/>
<connect gate="A" pin="1Q" pad="3"/>
<connect gate="A" pin="2D" pad="7"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="34C" pad="12"/>
<connect gate="A" pin="3D" pad="9"/>
<connect gate="A" pin="3Q" pad="11"/>
<connect gate="A" pin="4D" pad="15"/>
<connect gate="A" pin="4Q" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!1Q" pad="4"/>
<connect gate="A" pin="!2Q" pad="8"/>
<connect gate="A" pin="!3Q" pad="13"/>
<connect gate="A" pin="!4Q" pad="18"/>
<connect gate="A" pin="12C" pad="5"/>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="3"/>
<connect gate="A" pin="2D" pad="9"/>
<connect gate="A" pin="2Q" pad="7"/>
<connect gate="A" pin="34C" pad="15"/>
<connect gate="A" pin="3D" pad="12"/>
<connect gate="A" pin="3Q" pad="14"/>
<connect gate="A" pin="4D" pad="19"/>
<connect gate="A" pin="4Q" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*376" prefix="IC">
<description>Quadruple J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74376"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1J" pad="2"/>
<connect gate="A" pin="1K" pad="3"/>
<connect gate="A" pin="1Q" pad="4"/>
<connect gate="A" pin="2J" pad="7"/>
<connect gate="A" pin="2K" pad="6"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3J" pad="10"/>
<connect gate="A" pin="3K" pad="11"/>
<connect gate="A" pin="3Q" pad="12"/>
<connect gate="A" pin="4J" pad="15"/>
<connect gate="A" pin="4K" pad="14"/>
<connect gate="A" pin="4Q" pad="13"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1J" pad="2"/>
<connect gate="A" pin="1K" pad="3"/>
<connect gate="A" pin="1Q" pad="4"/>
<connect gate="A" pin="2J" pad="7"/>
<connect gate="A" pin="2K" pad="6"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3J" pad="10"/>
<connect gate="A" pin="3K" pad="11"/>
<connect gate="A" pin="3Q" pad="12"/>
<connect gate="A" pin="4J" pad="15"/>
<connect gate="A" pin="4K" pad="14"/>
<connect gate="A" pin="4Q" pad="13"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*377" prefix="IC">
<description>Octal D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, enable</description>
<gates>
<gate name="A" symbol="74377"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*378" prefix="IC">
<description>Hex D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, enable</description>
<gates>
<gate name="A" symbol="74378"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="6"/>
<connect gate="A" pin="3Q" pad="7"/>
<connect gate="A" pin="4D" pad="11"/>
<connect gate="A" pin="4Q" pad="10"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="6"/>
<connect gate="A" pin="3Q" pad="7"/>
<connect gate="A" pin="4D" pad="11"/>
<connect gate="A" pin="4Q" pad="10"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1D" pad="4"/>
<connect gate="A" pin="1Q" pad="3"/>
<connect gate="A" pin="2D" pad="5"/>
<connect gate="A" pin="2Q" pad="7"/>
<connect gate="A" pin="3D" pad="8"/>
<connect gate="A" pin="3Q" pad="9"/>
<connect gate="A" pin="4D" pad="14"/>
<connect gate="A" pin="4Q" pad="13"/>
<connect gate="A" pin="5D" pad="17"/>
<connect gate="A" pin="5Q" pad="15"/>
<connect gate="A" pin="6D" pad="18"/>
<connect gate="A" pin="6Q" pad="19"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="G" pad="2"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*379" prefix="IC">
<description>Quad D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, enable</description>
<gates>
<gate name="A" symbol="74379"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!1Q" pad="3"/>
<connect gate="A" pin="!2Q" pad="6"/>
<connect gate="A" pin="!3Q" pad="11"/>
<connect gate="A" pin="!4Q" pad="14"/>
<connect gate="A" pin="1D" pad="4"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="5"/>
<connect gate="A" pin="2Q" pad="7"/>
<connect gate="A" pin="3D" pad="12"/>
<connect gate="A" pin="3Q" pad="10"/>
<connect gate="A" pin="4D" pad="13"/>
<connect gate="A" pin="4Q" pad="15"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!1Q" pad="3"/>
<connect gate="A" pin="!2Q" pad="6"/>
<connect gate="A" pin="!3Q" pad="11"/>
<connect gate="A" pin="!4Q" pad="14"/>
<connect gate="A" pin="1D" pad="4"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="5"/>
<connect gate="A" pin="2Q" pad="7"/>
<connect gate="A" pin="3D" pad="12"/>
<connect gate="A" pin="3Q" pad="10"/>
<connect gate="A" pin="4D" pad="13"/>
<connect gate="A" pin="4Q" pad="15"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!1Q" pad="4"/>
<connect gate="A" pin="!2Q" pad="8"/>
<connect gate="A" pin="!3Q" pad="14"/>
<connect gate="A" pin="!4Q" pad="18"/>
<connect gate="A" pin="1D" pad="5"/>
<connect gate="A" pin="1Q" pad="3"/>
<connect gate="A" pin="2D" pad="7"/>
<connect gate="A" pin="2Q" pad="9"/>
<connect gate="A" pin="3D" pad="15"/>
<connect gate="A" pin="3Q" pad="13"/>
<connect gate="A" pin="4D" pad="17"/>
<connect gate="A" pin="4Q" pad="19"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="G" pad="2"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*381" prefix="IC">
<description>&lt;b&gt;ARITHMETIC LOGIC UNIT&lt;/b&gt; function generator</description>
<gates>
<gate name="A" symbol="74381"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A0" pad="3"/>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="19"/>
<connect gate="A" pin="A3" pad="17"/>
<connect gate="A" pin="B0" pad="4"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="18"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="CN" pad="15"/>
<connect gate="A" pin="F0" pad="8"/>
<connect gate="A" pin="F1" pad="9"/>
<connect gate="A" pin="F2" pad="11"/>
<connect gate="A" pin="F3" pad="12"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="P" pad="14"/>
<connect gate="A" pin="S0" pad="5"/>
<connect gate="A" pin="S1" pad="6"/>
<connect gate="A" pin="S2" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A0" pad="3"/>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="19"/>
<connect gate="A" pin="A3" pad="17"/>
<connect gate="A" pin="B0" pad="4"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="18"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="CN" pad="15"/>
<connect gate="A" pin="F0" pad="8"/>
<connect gate="A" pin="F1" pad="9"/>
<connect gate="A" pin="F2" pad="11"/>
<connect gate="A" pin="F3" pad="12"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="P" pad="14"/>
<connect gate="A" pin="S0" pad="5"/>
<connect gate="A" pin="S1" pad="6"/>
<connect gate="A" pin="S2" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A0" pad="3"/>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="19"/>
<connect gate="A" pin="A3" pad="17"/>
<connect gate="A" pin="B0" pad="4"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="18"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="CN" pad="15"/>
<connect gate="A" pin="F0" pad="8"/>
<connect gate="A" pin="F1" pad="9"/>
<connect gate="A" pin="F2" pad="11"/>
<connect gate="A" pin="F3" pad="12"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="P" pad="14"/>
<connect gate="A" pin="S0" pad="5"/>
<connect gate="A" pin="S1" pad="6"/>
<connect gate="A" pin="S2" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*382" prefix="IC">
<description>&lt;b&gt;ARITHMETIC LOGIC UNIT&lt;/b&gt; function generator</description>
<gates>
<gate name="A" symbol="74382"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A0" pad="3"/>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="19"/>
<connect gate="A" pin="A3" pad="17"/>
<connect gate="A" pin="B0" pad="4"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="18"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="CN" pad="15"/>
<connect gate="A" pin="CN+4" pad="14"/>
<connect gate="A" pin="F0" pad="8"/>
<connect gate="A" pin="F1" pad="9"/>
<connect gate="A" pin="F2" pad="11"/>
<connect gate="A" pin="F3" pad="12"/>
<connect gate="A" pin="OVR" pad="13"/>
<connect gate="A" pin="S0" pad="5"/>
<connect gate="A" pin="S1" pad="6"/>
<connect gate="A" pin="S2" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A0" pad="3"/>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="19"/>
<connect gate="A" pin="A3" pad="17"/>
<connect gate="A" pin="B0" pad="4"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="18"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="CN" pad="15"/>
<connect gate="A" pin="CN+4" pad="14"/>
<connect gate="A" pin="F0" pad="8"/>
<connect gate="A" pin="F1" pad="9"/>
<connect gate="A" pin="F2" pad="11"/>
<connect gate="A" pin="F3" pad="12"/>
<connect gate="A" pin="OVR" pad="13"/>
<connect gate="A" pin="S0" pad="5"/>
<connect gate="A" pin="S1" pad="6"/>
<connect gate="A" pin="S2" pad="7"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*384" prefix="IC">
<description>8-bit by 1 twos-complement &lt;b&gt;MULTIPLIER&lt;/b&gt;'</description>
<gates>
<gate name="A" symbol="74384"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="K" pad="10"/>
<connect gate="A" pin="MOD" pad="9"/>
<connect gate="A" pin="PRD" pad="6"/>
<connect gate="A" pin="X0" pad="5"/>
<connect gate="A" pin="X1" pad="4"/>
<connect gate="A" pin="X2" pad="3"/>
<connect gate="A" pin="X3" pad="2"/>
<connect gate="A" pin="X4" pad="14"/>
<connect gate="A" pin="X5" pad="13"/>
<connect gate="A" pin="X6" pad="12"/>
<connect gate="A" pin="X7" pad="11"/>
<connect gate="A" pin="Y" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*385" prefix="IC">
<description>Quadruple serial &lt;b&gt;ADDER/SUBTRACTOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74385"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1A" pad="5"/>
<connect gate="A" pin="1B" pad="4"/>
<connect gate="A" pin="1S" pad="2"/>
<connect gate="A" pin="1S/!A" pad="3"/>
<connect gate="A" pin="2A" pad="6"/>
<connect gate="A" pin="2B" pad="7"/>
<connect gate="A" pin="2S" pad="9"/>
<connect gate="A" pin="2S/!A" pad="8"/>
<connect gate="A" pin="3A" pad="15"/>
<connect gate="A" pin="3B" pad="14"/>
<connect gate="A" pin="3S" pad="12"/>
<connect gate="A" pin="3S/!A" pad="13"/>
<connect gate="A" pin="4A" pad="16"/>
<connect gate="A" pin="4B" pad="17"/>
<connect gate="A" pin="4S" pad="19"/>
<connect gate="A" pin="4S/!A" pad="18"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*390" prefix="IC">
<description>Dual 4-bit decade and binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74390"/>
<gate name="B" symbol="74390"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="5"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="B" pin="A" pad="15"/>
<connect gate="B" pin="B" pad="12"/>
<connect gate="B" pin="CLR" pad="14"/>
<connect gate="B" pin="QA" pad="13"/>
<connect gate="B" pin="QB" pad="11"/>
<connect gate="B" pin="QC" pad="10"/>
<connect gate="B" pin="QD" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="5"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="B" pin="A" pad="15"/>
<connect gate="B" pin="B" pad="12"/>
<connect gate="B" pin="CLR" pad="14"/>
<connect gate="B" pin="QA" pad="13"/>
<connect gate="B" pin="QB" pad="11"/>
<connect gate="B" pin="QC" pad="10"/>
<connect gate="B" pin="QD" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="QA" pad="4"/>
<connect gate="A" pin="QB" pad="7"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="B" pin="A" pad="19"/>
<connect gate="B" pin="B" pad="15"/>
<connect gate="B" pin="CLR" pad="18"/>
<connect gate="B" pin="QA" pad="17"/>
<connect gate="B" pin="QB" pad="14"/>
<connect gate="B" pin="QC" pad="13"/>
<connect gate="B" pin="QD" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*393" prefix="IC">
<description>Dual 4-bit decade and binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74393"/>
<gate name="B" symbol="74393"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="4"/>
<connect gate="A" pin="QC" pad="5"/>
<connect gate="A" pin="QD" pad="6"/>
<connect gate="B" pin="A" pad="13"/>
<connect gate="B" pin="CLR" pad="12"/>
<connect gate="B" pin="QA" pad="11"/>
<connect gate="B" pin="QB" pad="10"/>
<connect gate="B" pin="QC" pad="9"/>
<connect gate="B" pin="QD" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="4"/>
<connect gate="A" pin="QC" pad="5"/>
<connect gate="A" pin="QD" pad="6"/>
<connect gate="B" pin="A" pad="13"/>
<connect gate="B" pin="CLR" pad="12"/>
<connect gate="B" pin="QA" pad="11"/>
<connect gate="B" pin="QB" pad="10"/>
<connect gate="B" pin="QC" pad="9"/>
<connect gate="B" pin="QD" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="CLR" pad="3"/>
<connect gate="A" pin="QA" pad="4"/>
<connect gate="A" pin="QB" pad="6"/>
<connect gate="A" pin="QC" pad="8"/>
<connect gate="A" pin="QD" pad="9"/>
<connect gate="B" pin="A" pad="19"/>
<connect gate="B" pin="CLR" pad="18"/>
<connect gate="B" pin="QA" pad="16"/>
<connect gate="B" pin="QB" pad="14"/>
<connect gate="B" pin="QC" pad="13"/>
<connect gate="B" pin="QD" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*395" prefix="IC">
<description>4-bit cascadable &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74395"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="LD/!SH" pad="7"/>
<connect gate="A" pin="OC" pad="9"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="A" pin="QD*" pad="11"/>
<connect gate="A" pin="SER" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="LD/!SH" pad="7"/>
<connect gate="A" pin="OC" pad="9"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="14"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="12"/>
<connect gate="A" pin="QD*" pad="11"/>
<connect gate="A" pin="SER" pad="2"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="4"/>
<connect gate="A" pin="B" pad="5"/>
<connect gate="A" pin="C" pad="7"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="D" pad="8"/>
<connect gate="A" pin="LD/!SH" pad="9"/>
<connect gate="A" pin="OC" pad="12"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="18"/>
<connect gate="A" pin="QC" pad="17"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="QD*" pad="14"/>
<connect gate="A" pin="SER" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*396" prefix="IC">
<description>Octal storage &lt;b&gt;REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74396"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1Q1" pad="2"/>
<connect gate="A" pin="1Q2" pad="5"/>
<connect gate="A" pin="1Q3" pad="10"/>
<connect gate="A" pin="1Q4" pad="13"/>
<connect gate="A" pin="2Q1" pad="1"/>
<connect gate="A" pin="2Q2" pad="4"/>
<connect gate="A" pin="2Q3" pad="11"/>
<connect gate="A" pin="2Q4" pad="14"/>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="9"/>
<connect gate="A" pin="D4" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1Q1" pad="2"/>
<connect gate="A" pin="1Q2" pad="5"/>
<connect gate="A" pin="1Q3" pad="10"/>
<connect gate="A" pin="1Q4" pad="13"/>
<connect gate="A" pin="2Q1" pad="1"/>
<connect gate="A" pin="2Q2" pad="4"/>
<connect gate="A" pin="2Q3" pad="11"/>
<connect gate="A" pin="2Q4" pad="14"/>
<connect gate="A" pin="CLK" pad="7"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="9"/>
<connect gate="A" pin="D4" pad="12"/>
<connect gate="A" pin="G" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1Q1" pad="3"/>
<connect gate="A" pin="1Q2" pad="7"/>
<connect gate="A" pin="1Q3" pad="13"/>
<connect gate="A" pin="1Q4" pad="17"/>
<connect gate="A" pin="2Q1" pad="2"/>
<connect gate="A" pin="2Q2" pad="5"/>
<connect gate="A" pin="2Q3" pad="14"/>
<connect gate="A" pin="2Q4" pad="18"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="D1" pad="4"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="D3" pad="12"/>
<connect gate="A" pin="D4" pad="15"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*398" prefix="IC">
<description>Quadruple 2-input &lt;b&gt;MULTIPLEXER&lt;/b&gt;, storage</description>
<gates>
<gate name="A" symbol="74398"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="!QA" pad="3"/>
<connect gate="A" pin="!QB" pad="8"/>
<connect gate="A" pin="!QC" pad="13"/>
<connect gate="A" pin="!QD" pad="18"/>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="B1" pad="7"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="C1" pad="14"/>
<connect gate="A" pin="C2" pad="15"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="D1" pad="17"/>
<connect gate="A" pin="D2" pad="16"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="9"/>
<connect gate="A" pin="QC" pad="12"/>
<connect gate="A" pin="QD" pad="19"/>
<connect gate="A" pin="WS" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*399" prefix="IC">
<description>Quadruple 2-input &lt;b&gt;MULTIPLEXER&lt;/b&gt;, storage</description>
<gates>
<gate name="A" symbol="74399"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="B1" pad="6"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="C1" pad="11"/>
<connect gate="A" pin="C2" pad="12"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D2" pad="13"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="7"/>
<connect gate="A" pin="QC" pad="10"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="WS" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="B1" pad="6"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="C1" pad="11"/>
<connect gate="A" pin="C2" pad="12"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D2" pad="13"/>
<connect gate="A" pin="QA" pad="2"/>
<connect gate="A" pin="QB" pad="7"/>
<connect gate="A" pin="QC" pad="10"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="WS" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="B1" pad="8"/>
<connect gate="A" pin="B2" pad="7"/>
<connect gate="A" pin="C1" pad="14"/>
<connect gate="A" pin="C2" pad="15"/>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="D1" pad="18"/>
<connect gate="A" pin="D2" pad="17"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="9"/>
<connect gate="A" pin="QC" pad="13"/>
<connect gate="A" pin="QD" pad="19"/>
<connect gate="A" pin="WS" pad="2"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*412" prefix="IC">
<description>Multi mode buffered &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74412"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="DI1" pad="3"/>
<connect gate="A" pin="DI2" pad="5"/>
<connect gate="A" pin="DI3" pad="7"/>
<connect gate="A" pin="DI4" pad="9"/>
<connect gate="A" pin="DI5" pad="16"/>
<connect gate="A" pin="DI6" pad="18"/>
<connect gate="A" pin="DI7" pad="20"/>
<connect gate="A" pin="DI8" pad="22"/>
<connect gate="A" pin="DO1" pad="4"/>
<connect gate="A" pin="DO2" pad="6"/>
<connect gate="A" pin="DO3" pad="8"/>
<connect gate="A" pin="DO4" pad="10"/>
<connect gate="A" pin="DO5" pad="15"/>
<connect gate="A" pin="DO6" pad="17"/>
<connect gate="A" pin="DO7" pad="19"/>
<connect gate="A" pin="DO8" pad="21"/>
<connect gate="A" pin="INT" pad="23"/>
<connect gate="A" pin="M" pad="2"/>
<connect gate="A" pin="S1" pad="1"/>
<connect gate="A" pin="S2" pad="13"/>
<connect gate="A" pin="STB" pad="11"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*422" prefix="IC">
<description>Retriggerable monostable &lt;b&gt;MULTIVIBRATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74422"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="6"/>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="B1" pad="3"/>
<connect gate="A" pin="B2" pad="4"/>
<connect gate="A" pin="CLR" pad="5"/>
<connect gate="A" pin="CX" pad="11"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="RCX" pad="13"/>
<connect gate="A" pin="RI" pad="9"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*440" prefix="IC">
<description>Quadruple tridirectional &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74440"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*445" prefix="IC">
<description>BCD to decimal &lt;b&gt;DECODER/DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74445"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="14"/>
<connect gate="A" pin="C" pad="13"/>
<connect gate="A" pin="D" pad="12"/>
<connect gate="A" pin="O0" pad="1"/>
<connect gate="A" pin="O1" pad="2"/>
<connect gate="A" pin="O2" pad="3"/>
<connect gate="A" pin="O3" pad="4"/>
<connect gate="A" pin="O4" pad="5"/>
<connect gate="A" pin="O5" pad="6"/>
<connect gate="A" pin="O6" pad="7"/>
<connect gate="A" pin="O7" pad="9"/>
<connect gate="A" pin="O8" pad="10"/>
<connect gate="A" pin="O9" pad="11"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*446" prefix="IC">
<description>Quadruple &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74446"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="7"/>
<connect gate="A" pin="B1" pad="14"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="11"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="DR1" pad="13"/>
<connect gate="A" pin="DR2" pad="3"/>
<connect gate="A" pin="DR3" pad="6"/>
<connect gate="A" pin="DR4" pad="10"/>
<connect gate="A" pin="GAB" pad="15"/>
<connect gate="A" pin="GBA" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*449" prefix="IC">
<description>Quadruple &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74449"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="7"/>
<connect gate="A" pin="B1" pad="14"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="11"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="DR1" pad="13"/>
<connect gate="A" pin="DR2" pad="3"/>
<connect gate="A" pin="DR3" pad="6"/>
<connect gate="A" pin="DR4" pad="10"/>
<connect gate="A" pin="GAB" pad="15"/>
<connect gate="A" pin="GBA" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*465" prefix="IC">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74465"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="A7" pad="16"/>
<connect gate="A" pin="A8" pad="18"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="15"/>
<connect gate="A" pin="Y8" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*466" prefix="IC">
<description>Inverted octal &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74466"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="A7" pad="16"/>
<connect gate="A" pin="A8" pad="18"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="15"/>
<connect gate="A" pin="Y8" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="A7" pad="16"/>
<connect gate="A" pin="A8" pad="18"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="15"/>
<connect gate="A" pin="Y8" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*467" prefix="IC">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74467"/>
<gate name="B" symbol="74467"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="B" pin="A1" pad="12"/>
<connect gate="B" pin="A2" pad="14"/>
<connect gate="B" pin="A3" pad="16"/>
<connect gate="B" pin="A4" pad="18"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="11"/>
<connect gate="B" pin="Y2" pad="13"/>
<connect gate="B" pin="Y3" pad="15"/>
<connect gate="B" pin="Y4" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*468" prefix="IC">
<description>Inverted octal &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74468"/>
<gate name="B" symbol="74468"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="B" pin="A1" pad="12"/>
<connect gate="B" pin="A2" pad="14"/>
<connect gate="B" pin="A3" pad="16"/>
<connect gate="B" pin="A4" pad="18"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="11"/>
<connect gate="B" pin="Y2" pad="13"/>
<connect gate="B" pin="Y3" pad="15"/>
<connect gate="B" pin="Y4" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*490" prefix="IC">
<description>Dual 4-bit decade &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74490"/>
<gate name="B" symbol="74490"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CLR" pad="2"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="5"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="ST9" pad="4"/>
<connect gate="B" pin="CLK" pad="15"/>
<connect gate="B" pin="CLR" pad="14"/>
<connect gate="B" pin="QA" pad="13"/>
<connect gate="B" pin="QB" pad="11"/>
<connect gate="B" pin="QC" pad="10"/>
<connect gate="B" pin="QD" pad="9"/>
<connect gate="B" pin="ST9" pad="12"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*441" prefix="IC">
<description>4 bit tridirectional &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74440"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="J" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*442" prefix="IC">
<description>4 bit tridirectional &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74440"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="J" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*443" prefix="IC">
<description>4 bit tridirectional &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74440"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="J" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*444" prefix="IC">
<description>Quadruple tridirectional &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74440"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*448" prefix="IC">
<description>Quadruple tridirectional &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74440"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="A3" pad="14"/>
<connect gate="A" pin="A4" pad="13"/>
<connect gate="A" pin="B1" pad="2"/>
<connect gate="A" pin="B2" pad="5"/>
<connect gate="A" pin="B3" pad="6"/>
<connect gate="A" pin="B4" pad="9"/>
<connect gate="A" pin="C1" pad="3"/>
<connect gate="A" pin="C2" pad="4"/>
<connect gate="A" pin="C3" pad="7"/>
<connect gate="A" pin="C4" pad="8"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="GA" pad="17"/>
<connect gate="A" pin="GB" pad="18"/>
<connect gate="A" pin="GC" pad="19"/>
<connect gate="A" pin="S0" pad="11"/>
<connect gate="A" pin="S1" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*243" prefix="IC">
<description>Quadruple &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74243"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="10"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="B4" pad="8"/>
<connect gate="A" pin="GAB" pad="1"/>
<connect gate="A" pin="GBA" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="B1" pad="11"/>
<connect gate="A" pin="B2" pad="10"/>
<connect gate="A" pin="B3" pad="9"/>
<connect gate="A" pin="B4" pad="8"/>
<connect gate="A" pin="GAB" pad="1"/>
<connect gate="A" pin="GBA" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="6"/>
<connect gate="A" pin="A3" pad="8"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="B1" pad="16"/>
<connect gate="A" pin="B2" pad="14"/>
<connect gate="A" pin="B3" pad="13"/>
<connect gate="A" pin="B4" pad="12"/>
<connect gate="A" pin="GAB" pad="2"/>
<connect gate="A" pin="GBA" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*06" prefix="IC">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;, open collector high-voltage output</description>
<gates>
<gate name="A" symbol="7405"/>
<gate name="B" symbol="7405"/>
<gate name="C" symbol="7405"/>
<gate name="D" symbol="7405"/>
<gate name="E" symbol="7405"/>
<gate name="F" symbol="7405"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I" pad="4"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="12"/>
<connect gate="E" pin="I" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I" pad="19"/>
<connect gate="F" pin="O" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*282" prefix="IC">
<description>&lt;b&gt;LOOK AHEAD CARRY GENERATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74282"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="CN*" pad="13"/>
<connect gate="A" pin="CN+X" pad="15"/>
<connect gate="A" pin="CN+Y" pad="14"/>
<connect gate="A" pin="CN+Z" pad="11"/>
<connect gate="A" pin="CNA" pad="17"/>
<connect gate="A" pin="CNB" pad="16"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="G0" pad="3"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="18"/>
<connect gate="A" pin="G3" pad="5"/>
<connect gate="A" pin="P" pad="9"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="2"/>
<connect gate="A" pin="P2" pad="19"/>
<connect gate="A" pin="P3" pad="6"/>
<connect gate="A" pin="S0" pad="7"/>
<connect gate="A" pin="S1" pad="8"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*00" prefix="IC">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7400"/>
<gate name="B" symbol="7400"/>
<gate name="C" symbol="7400"/>
<gate name="D" symbol="7400"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*01" prefix="IC">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; gate, open collector</description>
<gates>
<gate name="A" symbol="7401"/>
<gate name="B" symbol="7401"/>
<gate name="C" symbol="7401"/>
<gate name="D" symbol="7401"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="11"/>
<connect gate="D" pin="I1" pad="12"/>
<connect gate="D" pin="O" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="11"/>
<connect gate="D" pin="I1" pad="12"/>
<connect gate="D" pin="O" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="3"/>
<connect gate="A" pin="I1" pad="4"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="8"/>
<connect gate="B" pin="I1" pad="9"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="12"/>
<connect gate="C" pin="I1" pad="13"/>
<connect gate="C" pin="O" pad="14"/>
<connect gate="D" pin="I0" pad="16"/>
<connect gate="D" pin="I1" pad="18"/>
<connect gate="D" pin="O" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*02" prefix="IC">
<description>Quad 2-input &lt;b&gt;NOR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7402"/>
<gate name="B" symbol="7402"/>
<gate name="C" symbol="7402"/>
<gate name="D" symbol="7402"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="11"/>
<connect gate="D" pin="I1" pad="12"/>
<connect gate="D" pin="O" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="11"/>
<connect gate="D" pin="I1" pad="12"/>
<connect gate="D" pin="O" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="3"/>
<connect gate="A" pin="I1" pad="4"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="8"/>
<connect gate="B" pin="I1" pad="9"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="12"/>
<connect gate="C" pin="I1" pad="13"/>
<connect gate="C" pin="O" pad="14"/>
<connect gate="D" pin="I0" pad="16"/>
<connect gate="D" pin="I1" pad="18"/>
<connect gate="D" pin="O" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*03" prefix="IC">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; gate, open collector output</description>
<gates>
<gate name="A" symbol="7403"/>
<gate name="B" symbol="7403"/>
<gate name="C" symbol="7403"/>
<gate name="D" symbol="7403"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*08" prefix="IC">
<description>Quad 2-input &lt;b&gt;AND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7408"/>
<gate name="B" symbol="7408"/>
<gate name="C" symbol="7408"/>
<gate name="D" symbol="7408"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*09" prefix="IC">
<description>Quad 2-input &lt;b&gt;AND&lt;/b&gt; gate, open collector</description>
<gates>
<gate name="A" symbol="7409"/>
<gate name="B" symbol="7409"/>
<gate name="C" symbol="7409"/>
<gate name="D" symbol="7409"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*10" prefix="IC">
<description>Triple 3-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7410"/>
<gate name="B" symbol="7410"/>
<gate name="C" symbol="7410"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="19"/>
<connect gate="A" pin="O" pad="18"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="I2" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="I2" pad="16"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*11" prefix="IC">
<description>Triple 3-input &lt;b&gt;AND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7411"/>
<gate name="B" symbol="7411"/>
<gate name="C" symbol="7411"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="19"/>
<connect gate="A" pin="O" pad="18"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="I2" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="I2" pad="16"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*12" prefix="IC">
<description>Triple 3-input &lt;b&gt;NAND&lt;/b&gt; gate, open collector</description>
<gates>
<gate name="A" symbol="7412"/>
<gate name="B" symbol="7412"/>
<gate name="C" symbol="7412"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*13" prefix="IC">
<description>Dual 4-input &lt;b&gt;NAND&lt;/b&gt; schmitt trigger</description>
<gates>
<gate name="A" symbol="7413"/>
<gate name="B" symbol="7413"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="B" pin="I0" pad="9"/>
<connect gate="B" pin="I1" pad="10"/>
<connect gate="B" pin="I2" pad="12"/>
<connect gate="B" pin="I3" pad="13"/>
<connect gate="B" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*15" prefix="IC">
<description>Triple 3-input &lt;b&gt;AND&lt;/b&gt; gate, open collector</description>
<gates>
<gate name="A" symbol="7415"/>
<gate name="B" symbol="7415"/>
<gate name="C" symbol="7415"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*21" prefix="IC">
<description>Dual 4-input &lt;b&gt;AND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7421"/>
<gate name="B" symbol="7421"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="B" pin="I0" pad="9"/>
<connect gate="B" pin="I1" pad="10"/>
<connect gate="B" pin="I2" pad="12"/>
<connect gate="B" pin="I3" pad="13"/>
<connect gate="B" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="B" pin="I0" pad="9"/>
<connect gate="B" pin="I1" pad="10"/>
<connect gate="B" pin="I2" pad="12"/>
<connect gate="B" pin="I3" pad="13"/>
<connect gate="B" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="6"/>
<connect gate="A" pin="I3" pad="8"/>
<connect gate="A" pin="O" pad="9"/>
<connect gate="B" pin="I0" pad="13"/>
<connect gate="B" pin="I1" pad="14"/>
<connect gate="B" pin="I2" pad="18"/>
<connect gate="B" pin="I3" pad="19"/>
<connect gate="B" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*22" prefix="IC">
<description>Dual 4-input &lt;b&gt;NAND&lt;/b&gt; gate, open collector</description>
<gates>
<gate name="A" symbol="7422"/>
<gate name="B" symbol="7422"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="B" pin="I0" pad="9"/>
<connect gate="B" pin="I1" pad="10"/>
<connect gate="B" pin="I2" pad="12"/>
<connect gate="B" pin="I3" pad="13"/>
<connect gate="B" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*25" prefix="IC">
<description>Dual 4-input &lt;b&gt;NOR&lt;/b&gt; gate, strobe</description>
<gates>
<gate name="A" symbol="7425"/>
<gate name="B" symbol="7425"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="B" pin="G" pad="11"/>
<connect gate="B" pin="I0" pad="9"/>
<connect gate="B" pin="I1" pad="10"/>
<connect gate="B" pin="I2" pad="12"/>
<connect gate="B" pin="I3" pad="13"/>
<connect gate="B" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="B" pin="G" pad="11"/>
<connect gate="B" pin="I0" pad="9"/>
<connect gate="B" pin="I1" pad="10"/>
<connect gate="B" pin="I2" pad="12"/>
<connect gate="B" pin="I3" pad="13"/>
<connect gate="B" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*27" prefix="IC">
<description>Triple 3-input &lt;b&gt;NOR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7427"/>
<gate name="B" symbol="7427"/>
<gate name="C" symbol="7427"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I0" pad="3"/>
<connect gate="B" pin="I1" pad="4"/>
<connect gate="B" pin="I2" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="I2" pad="11"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="19"/>
<connect gate="A" pin="O" pad="18"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="I2" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="I2" pad="16"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*30" prefix="IC">
<description>8-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7430"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="4"/>
<connect gate="A" pin="I4" pad="5"/>
<connect gate="A" pin="I5" pad="6"/>
<connect gate="A" pin="I6" pad="11"/>
<connect gate="A" pin="I7" pad="12"/>
<connect gate="A" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="4"/>
<connect gate="A" pin="I4" pad="5"/>
<connect gate="A" pin="I5" pad="6"/>
<connect gate="A" pin="I6" pad="11"/>
<connect gate="A" pin="I7" pad="12"/>
<connect gate="A" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="6"/>
<connect gate="A" pin="I4" pad="8"/>
<connect gate="A" pin="I5" pad="9"/>
<connect gate="A" pin="I6" pad="16"/>
<connect gate="A" pin="I7" pad="18"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*32" prefix="IC">
<description>Quad 2-input &lt;b&gt;OR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7432"/>
<gate name="B" symbol="7432"/>
<gate name="C" symbol="7432"/>
<gate name="D" symbol="7432"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*33" prefix="IC">
<description>Quad 2-input &lt;b&gt;NOR&lt;/b&gt; buffer, open collector</description>
<gates>
<gate name="A" symbol="7433"/>
<gate name="B" symbol="7433"/>
<gate name="C" symbol="7433"/>
<gate name="D" symbol="7433"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="11"/>
<connect gate="D" pin="I1" pad="12"/>
<connect gate="D" pin="O" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="11"/>
<connect gate="D" pin="I1" pad="12"/>
<connect gate="D" pin="O" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="3"/>
<connect gate="A" pin="I1" pad="4"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I0" pad="8"/>
<connect gate="B" pin="I1" pad="9"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="12"/>
<connect gate="C" pin="I1" pad="13"/>
<connect gate="C" pin="O" pad="14"/>
<connect gate="D" pin="I0" pad="16"/>
<connect gate="D" pin="I1" pad="18"/>
<connect gate="D" pin="O" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*39" prefix="IC">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; buffer, open collector</description>
<gates>
<gate name="A" symbol="7439"/>
<gate name="B" symbol="7439"/>
<gate name="C" symbol="7439"/>
<gate name="D" symbol="7439"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="1"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="11"/>
<connect gate="D" pin="I1" pad="12"/>
<connect gate="D" pin="O" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*65" prefix="IC">
<description>4-2-3-2 input &lt;b&gt;AND OR INVERTER&lt;/b&gt; gates</description>
<gates>
<gate name="A" symbol="7465"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="11"/>
<connect gate="A" pin="I10" pad="10"/>
<connect gate="A" pin="I2" pad="12"/>
<connect gate="A" pin="I3" pad="13"/>
<connect gate="A" pin="I4" pad="2"/>
<connect gate="A" pin="I5" pad="3"/>
<connect gate="A" pin="I6" pad="4"/>
<connect gate="A" pin="I7" pad="5"/>
<connect gate="A" pin="I8" pad="6"/>
<connect gate="A" pin="I9" pad="9"/>
<connect gate="A" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*86" prefix="IC">
<description>Quad 2-input &lt;b&gt;EXCLUSIV-OR (XOR)&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7486"/>
<gate name="B" symbol="7486"/>
<gate name="C" symbol="7486"/>
<gate name="D" symbol="7486"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*125" prefix="IC">
<description>Quad bus &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74125"/>
<gate name="B" symbol="74125"/>
<gate name="C" symbol="74125"/>
<gate name="D" symbol="74125"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="PW" package="TSSOP14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ABT"/>
</technologies>
</device>
<device name="DB" package="SSOP14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ABT"/>
</technologies>
</device>
<device name="BQ" package="DHVQFN14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ABT"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*126" prefix="IC">
<description>Quad bus &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74126"/>
<gate name="B" symbol="74126"/>
<gate name="C" symbol="74126"/>
<gate name="D" symbol="74126"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="B" pin="OE" pad="4"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="C" pin="OE" pad="10"/>
<connect gate="D" pin="I" pad="12"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="D" pin="OE" pad="13"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="A" pin="OE" pad="2"/>
<connect gate="B" pin="I" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="B" pin="OE" pad="6"/>
<connect gate="C" pin="I" pad="13"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="C" pin="OE" pad="14"/>
<connect gate="D" pin="I" pad="18"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="D" pin="OE" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*133" prefix="IC">
<description>13-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="74133"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I10" pad="13"/>
<connect gate="A" pin="I11" pad="14"/>
<connect gate="A" pin="I12" pad="15"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="4"/>
<connect gate="A" pin="I4" pad="5"/>
<connect gate="A" pin="I5" pad="6"/>
<connect gate="A" pin="I6" pad="7"/>
<connect gate="A" pin="I7" pad="10"/>
<connect gate="A" pin="I8" pad="11"/>
<connect gate="A" pin="I9" pad="12"/>
<connect gate="A" pin="O" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I10" pad="13"/>
<connect gate="A" pin="I11" pad="14"/>
<connect gate="A" pin="I12" pad="15"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="4"/>
<connect gate="A" pin="I4" pad="5"/>
<connect gate="A" pin="I5" pad="6"/>
<connect gate="A" pin="I6" pad="7"/>
<connect gate="A" pin="I7" pad="10"/>
<connect gate="A" pin="I8" pad="11"/>
<connect gate="A" pin="I9" pad="12"/>
<connect gate="A" pin="O" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I10" pad="17"/>
<connect gate="A" pin="I11" pad="18"/>
<connect gate="A" pin="I12" pad="19"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="I4" pad="7"/>
<connect gate="A" pin="I5" pad="8"/>
<connect gate="A" pin="I6" pad="9"/>
<connect gate="A" pin="I7" pad="13"/>
<connect gate="A" pin="I8" pad="14"/>
<connect gate="A" pin="I9" pad="15"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*134" prefix="IC">
<description>12-input &lt;b&gt;NAND&lt;/b&gt; gate, 3-stage</description>
<gates>
<gate name="A" symbol="74134"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I10" pad="13"/>
<connect gate="A" pin="I11" pad="14"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="4"/>
<connect gate="A" pin="I4" pad="5"/>
<connect gate="A" pin="I5" pad="6"/>
<connect gate="A" pin="I6" pad="7"/>
<connect gate="A" pin="I7" pad="10"/>
<connect gate="A" pin="I8" pad="11"/>
<connect gate="A" pin="I9" pad="12"/>
<connect gate="A" pin="O" pad="9"/>
<connect gate="A" pin="OE" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*135" prefix="IC">
<description>Quad &lt;b&gt;EXCLUSIV-OR/NOR (XOR/NOR)&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="74135"/>
<gate name="B" symbol="74135"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="1A" pad="1"/>
<connect gate="A" pin="1B" pad="2"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="B" pin="1A" pad="10"/>
<connect gate="B" pin="1B" pad="11"/>
<connect gate="B" pin="1Y" pad="9"/>
<connect gate="B" pin="2A" pad="14"/>
<connect gate="B" pin="2B" pad="15"/>
<connect gate="B" pin="2Y" pad="13"/>
<connect gate="B" pin="C" pad="12"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="1A" pad="1"/>
<connect gate="A" pin="1B" pad="2"/>
<connect gate="A" pin="1Y" pad="3"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="C" pad="4"/>
<connect gate="B" pin="1A" pad="10"/>
<connect gate="B" pin="1B" pad="11"/>
<connect gate="B" pin="1Y" pad="9"/>
<connect gate="B" pin="2A" pad="14"/>
<connect gate="B" pin="2B" pad="15"/>
<connect gate="B" pin="2Y" pad="13"/>
<connect gate="B" pin="C" pad="12"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="7"/>
<connect gate="A" pin="2B" pad="8"/>
<connect gate="A" pin="2Y" pad="9"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="B" pin="1A" pad="13"/>
<connect gate="B" pin="1B" pad="14"/>
<connect gate="B" pin="1Y" pad="12"/>
<connect gate="B" pin="2A" pad="18"/>
<connect gate="B" pin="2B" pad="19"/>
<connect gate="B" pin="2Y" pad="17"/>
<connect gate="B" pin="C" pad="15"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*136" prefix="IC">
<description>Quad &lt;b&gt;EXCLUSIV-OR/NOR (XOR/NOR)&lt;/b&gt; gate, open collector</description>
<gates>
<gate name="A" symbol="74136"/>
<gate name="B" symbol="74136"/>
<gate name="C" symbol="74136"/>
<gate name="D" symbol="74136"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*260" prefix="IC">
<description>Dual 5-input positive &lt;b&gt;NOR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="74260"/>
<gate name="B" symbol="74260"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="12"/>
<connect gate="A" pin="I4" pad="13"/>
<connect gate="A" pin="O" pad="5"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="I2" pad="9"/>
<connect gate="B" pin="I3" pad="10"/>
<connect gate="B" pin="I4" pad="11"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="3"/>
<connect gate="A" pin="I3" pad="12"/>
<connect gate="A" pin="I4" pad="13"/>
<connect gate="A" pin="O" pad="5"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="I2" pad="9"/>
<connect gate="B" pin="I3" pad="10"/>
<connect gate="B" pin="I4" pad="11"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="18"/>
<connect gate="A" pin="I4" pad="19"/>
<connect gate="A" pin="O" pad="8"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="12"/>
<connect gate="B" pin="I2" pad="13"/>
<connect gate="B" pin="I3" pad="14"/>
<connect gate="B" pin="I4" pad="16"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*266" prefix="IC">
<description>Quadruple &lt;b&gt;EXCLUSIVE-NOR (XNOR)&lt;/b&gt;, open-collector</description>
<gates>
<gate name="A" symbol="74266"/>
<gate name="B" symbol="74266"/>
<gate name="C" symbol="74266"/>
<gate name="D" symbol="74266"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="8"/>
<connect gate="B" pin="I1" pad="9"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="12"/>
<connect gate="C" pin="I1" pad="13"/>
<connect gate="C" pin="O" pad="14"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*386" prefix="IC">
<description>Quadruple 2-input &lt;b&gt;EXCLUSIVE-OR (XOR)&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="74386"/>
<gate name="B" symbol="74386"/>
<gate name="C" symbol="74386"/>
<gate name="D" symbol="74386"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="5"/>
<connect gate="B" pin="I1" pad="6"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I0" pad="8"/>
<connect gate="C" pin="I1" pad="9"/>
<connect gate="C" pin="O" pad="10"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*14" prefix="IC">
<description>Hex schmitt trigger &lt;b&gt;INVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7414"/>
<gate name="B" symbol="7414"/>
<gate name="C" symbol="7414"/>
<gate name="D" symbol="7414"/>
<gate name="E" symbol="7414"/>
<gate name="F" symbol="7414"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I" pad="11"/>
<connect gate="B" pin="O" pad="10"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I" pad="1"/>
<connect gate="D" pin="O" pad="2"/>
<connect gate="E" pin="I" pad="3"/>
<connect gate="E" pin="O" pad="4"/>
<connect gate="F" pin="I" pad="5"/>
<connect gate="F" pin="O" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I" pad="11"/>
<connect gate="B" pin="O" pad="10"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I" pad="1"/>
<connect gate="D" pin="O" pad="2"/>
<connect gate="E" pin="I" pad="3"/>
<connect gate="E" pin="O" pad="4"/>
<connect gate="F" pin="I" pad="5"/>
<connect gate="F" pin="O" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I" pad="4"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I" pad="13"/>
<connect gate="D" pin="O" pad="12"/>
<connect gate="E" pin="I" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I" pad="19"/>
<connect gate="F" pin="O" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*26" prefix="IC">
<description>Quad 2-input high voltage interface &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7403"/>
<gate name="B" symbol="7403"/>
<gate name="C" symbol="7403"/>
<gate name="D" symbol="7403"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*132" prefix="IC">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; schmitt trigger</description>
<gates>
<gate name="A" symbol="74132"/>
<gate name="B" symbol="74132"/>
<gate name="C" symbol="74132"/>
<gate name="D" symbol="74132"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*518" prefix="IC">
<description>8-bit &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74518"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*520" prefix="IC">
<description>8-bit &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74520"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*522" prefix="IC">
<description>8-bit &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74522"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*526" prefix="IC">
<description>16-bit programmable &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74526"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="3"/>
<connect gate="A" pin="P10" pad="13"/>
<connect gate="A" pin="P11" pad="14"/>
<connect gate="A" pin="P12" pad="15"/>
<connect gate="A" pin="P13" pad="16"/>
<connect gate="A" pin="P14" pad="17"/>
<connect gate="A" pin="P15" pad="18"/>
<connect gate="A" pin="P2" pad="4"/>
<connect gate="A" pin="P3" pad="5"/>
<connect gate="A" pin="P4" pad="6"/>
<connect gate="A" pin="P5" pad="7"/>
<connect gate="A" pin="P6" pad="8"/>
<connect gate="A" pin="P7" pad="9"/>
<connect gate="A" pin="P8" pad="11"/>
<connect gate="A" pin="P9" pad="12"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*527" prefix="IC">
<description>12-bit prorammable &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74527"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="3"/>
<connect gate="A" pin="P10" pad="15"/>
<connect gate="A" pin="P11" pad="17"/>
<connect gate="A" pin="P2" pad="4"/>
<connect gate="A" pin="P3" pad="5"/>
<connect gate="A" pin="P4" pad="6"/>
<connect gate="A" pin="P5" pad="7"/>
<connect gate="A" pin="P6" pad="8"/>
<connect gate="A" pin="P7" pad="9"/>
<connect gate="A" pin="P8" pad="11"/>
<connect gate="A" pin="P9" pad="13"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="Q10" pad="16"/>
<connect gate="A" pin="Q11" pad="18"/>
<connect gate="A" pin="Q8" pad="12"/>
<connect gate="A" pin="Q9" pad="14"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*528" prefix="IC">
<description>12-bit programmable &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74528"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="3"/>
<connect gate="A" pin="P10" pad="13"/>
<connect gate="A" pin="P11" pad="14"/>
<connect gate="A" pin="P2" pad="4"/>
<connect gate="A" pin="P3" pad="5"/>
<connect gate="A" pin="P4" pad="6"/>
<connect gate="A" pin="P5" pad="7"/>
<connect gate="A" pin="P6" pad="9"/>
<connect gate="A" pin="P7" pad="10"/>
<connect gate="A" pin="P8" pad="11"/>
<connect gate="A" pin="P9" pad="12"/>
<connect gate="A" pin="P=Q" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*540" prefix="IC">
<description>Inverting Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74540"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*541" prefix="IC">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74541"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*560" prefix="IC">
<description>Synchronous decade &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74560"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="ACL" pad="8"/>
<connect gate="A" pin="ALD" pad="1"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CCO" pad="18"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="12"/>
<connect gate="A" pin="G" pad="17"/>
<connect gate="A" pin="QA" pad="16"/>
<connect gate="A" pin="QB" pad="15"/>
<connect gate="A" pin="QC" pad="14"/>
<connect gate="A" pin="QD" pad="13"/>
<connect gate="A" pin="RCO" pad="19"/>
<connect gate="A" pin="SCL" pad="9"/>
<connect gate="A" pin="SLD" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*568" prefix="IC">
<description>Synchronous decade &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74568"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="ACLR" pad="8"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CCO" pad="18"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="12"/>
<connect gate="A" pin="G" pad="17"/>
<connect gate="A" pin="LOAD" pad="11"/>
<connect gate="A" pin="QA" pad="16"/>
<connect gate="A" pin="QB" pad="15"/>
<connect gate="A" pin="QC" pad="14"/>
<connect gate="A" pin="QD" pad="13"/>
<connect gate="A" pin="RCO" pad="19"/>
<connect gate="A" pin="SCLR" pad="9"/>
<connect gate="A" pin="U/!D" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*589" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, input latch, 3-state</description>
<gates>
<gate name="A" symbol="74589"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="E" pad="4"/>
<connect gate="A" pin="F" pad="5"/>
<connect gate="A" pin="G" pad="6"/>
<connect gate="A" pin="H" pad="7"/>
<connect gate="A" pin="OC" pad="10"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="SRCK" pad="11"/>
<connect gate="A" pin="SRLD" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*590" prefix="IC">
<description>8-bit binary &lt;b&gt;COUNTER&lt;/b&gt;, output register</description>
<gates>
<gate name="A" symbol="74590"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CCKEN" pad="12"/>
<connect gate="A" pin="CCLR" pad="10"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="RCK" pad="13"/>
<connect gate="A" pin="RCO" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="CCKEN" pad="12"/>
<connect gate="A" pin="CCLR" pad="10"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="RCK" pad="13"/>
<connect gate="A" pin="RCO" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="CCKEN" pad="15"/>
<connect gate="A" pin="CCLR" pad="13"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="G" pad="18"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="3"/>
<connect gate="A" pin="QD" pad="4"/>
<connect gate="A" pin="QE" pad="5"/>
<connect gate="A" pin="QF" pad="7"/>
<connect gate="A" pin="QG" pad="8"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="RCK" pad="17"/>
<connect gate="A" pin="RCO" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*591" prefix="IC">
<description>8-bit binary &lt;b&gt;COUNTER&lt;/b&gt;, output register</description>
<gates>
<gate name="A" symbol="74591"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CCKEN" pad="12"/>
<connect gate="A" pin="CCLR" pad="10"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="G" pad="14"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="RCK" pad="13"/>
<connect gate="A" pin="RCO" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*592" prefix="IC">
<description>8-bit binary &lt;b&gt;COUNTER&lt;/b&gt;, input register</description>
<gates>
<gate name="A" symbol="74592"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="A" pin="CCK" pad="11"/>
<connect gate="A" pin="CCKEN" pad="12"/>
<connect gate="A" pin="CCL" pad="10"/>
<connect gate="A" pin="CLD" pad="14"/>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="E" pad="4"/>
<connect gate="A" pin="F" pad="5"/>
<connect gate="A" pin="G" pad="6"/>
<connect gate="A" pin="H" pad="7"/>
<connect gate="A" pin="RCK" pad="13"/>
<connect gate="A" pin="RCO" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="A" pin="CCK" pad="11"/>
<connect gate="A" pin="CCKEN" pad="12"/>
<connect gate="A" pin="CCL" pad="10"/>
<connect gate="A" pin="CLD" pad="14"/>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="E" pad="4"/>
<connect gate="A" pin="F" pad="5"/>
<connect gate="A" pin="G" pad="6"/>
<connect gate="A" pin="H" pad="7"/>
<connect gate="A" pin="RCK" pad="13"/>
<connect gate="A" pin="RCO" pad="9"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="19"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="CCK" pad="14"/>
<connect gate="A" pin="CCKEN" pad="15"/>
<connect gate="A" pin="CCL" pad="13"/>
<connect gate="A" pin="CLD" pad="18"/>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="E" pad="5"/>
<connect gate="A" pin="F" pad="7"/>
<connect gate="A" pin="G" pad="8"/>
<connect gate="A" pin="H" pad="9"/>
<connect gate="A" pin="RCK" pad="17"/>
<connect gate="A" pin="RCO" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*593" prefix="IC">
<description>8-bit binary &lt;b&gt;COUNTER&lt;/b&gt;, input register</description>
<gates>
<gate name="A" symbol="74593"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="!CCKEN" pad="14"/>
<connect gate="A" pin="!G" pad="18"/>
<connect gate="A" pin="A/QA" pad="1"/>
<connect gate="A" pin="B/QB" pad="2"/>
<connect gate="A" pin="C/QC" pad="3"/>
<connect gate="A" pin="CCK" pad="13"/>
<connect gate="A" pin="CCKEN" pad="15"/>
<connect gate="A" pin="CCLR" pad="12"/>
<connect gate="A" pin="CLOAD" pad="9"/>
<connect gate="A" pin="D/QD" pad="4"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="6"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="A" pin="G/QG" pad="7"/>
<connect gate="A" pin="H/QH" pad="8"/>
<connect gate="A" pin="RCK" pad="16"/>
<connect gate="A" pin="RCKEN" pad="17"/>
<connect gate="A" pin="RCO" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="!CCKEN" pad="14"/>
<connect gate="A" pin="!G" pad="18"/>
<connect gate="A" pin="A/QA" pad="1"/>
<connect gate="A" pin="B/QB" pad="2"/>
<connect gate="A" pin="C/QC" pad="3"/>
<connect gate="A" pin="CCK" pad="13"/>
<connect gate="A" pin="CCKEN" pad="15"/>
<connect gate="A" pin="CCLR" pad="12"/>
<connect gate="A" pin="CLOAD" pad="9"/>
<connect gate="A" pin="D/QD" pad="4"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="6"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="A" pin="G/QG" pad="7"/>
<connect gate="A" pin="H/QH" pad="8"/>
<connect gate="A" pin="RCK" pad="16"/>
<connect gate="A" pin="RCKEN" pad="17"/>
<connect gate="A" pin="RCO" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="!CCKEN" pad="14"/>
<connect gate="A" pin="!G" pad="18"/>
<connect gate="A" pin="A/QA" pad="1"/>
<connect gate="A" pin="B/QB" pad="2"/>
<connect gate="A" pin="C/QC" pad="3"/>
<connect gate="A" pin="CCK" pad="13"/>
<connect gate="A" pin="CCKEN" pad="15"/>
<connect gate="A" pin="CCLR" pad="12"/>
<connect gate="A" pin="CLOAD" pad="9"/>
<connect gate="A" pin="D/QD" pad="4"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="6"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="A" pin="G/QG" pad="7"/>
<connect gate="A" pin="H/QH" pad="8"/>
<connect gate="A" pin="RCK" pad="16"/>
<connect gate="A" pin="RCKEN" pad="17"/>
<connect gate="A" pin="RCO" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*594" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch</description>
<gates>
<gate name="A" symbol="74594"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="RCL" pad="13"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="RCL" pad="13"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*595" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch</description>
<gates>
<gate name="A" symbol="74595"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="G" pad="17"/>
<connect gate="A" pin="QA" pad="19"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="3"/>
<connect gate="A" pin="QD" pad="4"/>
<connect gate="A" pin="QE" pad="5"/>
<connect gate="A" pin="QF" pad="7"/>
<connect gate="A" pin="QG" pad="8"/>
<connect gate="A" pin="QH" pad="9"/>
<connect gate="A" pin="QH*" pad="12"/>
<connect gate="A" pin="RCK" pad="15"/>
<connect gate="A" pin="SCK" pad="14"/>
<connect gate="A" pin="SCL" pad="13"/>
<connect gate="A" pin="SER" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*596" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch, open collector</description>
<gates>
<gate name="A" symbol="74596"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="G" pad="13"/>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*597" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, input latch</description>
<gates>
<gate name="A" symbol="74597"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="E" pad="4"/>
<connect gate="A" pin="F" pad="5"/>
<connect gate="A" pin="G" pad="6"/>
<connect gate="A" pin="H" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="SLD" pad="13"/>
<connect gate="A" pin="SRCK" pad="11"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="A" pin="D" pad="3"/>
<connect gate="A" pin="E" pad="4"/>
<connect gate="A" pin="F" pad="5"/>
<connect gate="A" pin="G" pad="6"/>
<connect gate="A" pin="H" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="A" pin="SLD" pad="13"/>
<connect gate="A" pin="SRCK" pad="11"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="19"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="D" pad="4"/>
<connect gate="A" pin="E" pad="5"/>
<connect gate="A" pin="F" pad="7"/>
<connect gate="A" pin="G" pad="8"/>
<connect gate="A" pin="H" pad="9"/>
<connect gate="A" pin="QH*" pad="12"/>
<connect gate="A" pin="RCK" pad="15"/>
<connect gate="A" pin="SCL" pad="13"/>
<connect gate="A" pin="SER" pad="18"/>
<connect gate="A" pin="SLD" pad="17"/>
<connect gate="A" pin="SRCK" pad="14"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*598" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, input latch</description>
<gates>
<gate name="A" symbol="74598"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A/QA" pad="1"/>
<connect gate="A" pin="B/QB" pad="2"/>
<connect gate="A" pin="C/QC" pad="3"/>
<connect gate="A" pin="D/QD" pad="4"/>
<connect gate="A" pin="DS" pad="19"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="6"/>
<connect gate="A" pin="G" pad="16"/>
<connect gate="A" pin="G/QG" pad="7"/>
<connect gate="A" pin="H/QH" pad="8"/>
<connect gate="A" pin="QH*" pad="11"/>
<connect gate="A" pin="RCK" pad="15"/>
<connect gate="A" pin="SCK" pad="13"/>
<connect gate="A" pin="SCKE" pad="14"/>
<connect gate="A" pin="SCL" pad="12"/>
<connect gate="A" pin="SLD" pad="9"/>
<connect gate="A" pin="SR0" pad="18"/>
<connect gate="A" pin="SR1" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A/QA" pad="1"/>
<connect gate="A" pin="B/QB" pad="2"/>
<connect gate="A" pin="C/QC" pad="3"/>
<connect gate="A" pin="D/QD" pad="4"/>
<connect gate="A" pin="DS" pad="19"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="6"/>
<connect gate="A" pin="G" pad="16"/>
<connect gate="A" pin="G/QG" pad="7"/>
<connect gate="A" pin="H/QH" pad="8"/>
<connect gate="A" pin="QH*" pad="11"/>
<connect gate="A" pin="RCK" pad="15"/>
<connect gate="A" pin="SCK" pad="13"/>
<connect gate="A" pin="SCKE" pad="14"/>
<connect gate="A" pin="SCL" pad="12"/>
<connect gate="A" pin="SLD" pad="9"/>
<connect gate="A" pin="SR0" pad="18"/>
<connect gate="A" pin="SR1" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A/QA" pad="1"/>
<connect gate="A" pin="B/QB" pad="2"/>
<connect gate="A" pin="C/QC" pad="3"/>
<connect gate="A" pin="D/QD" pad="4"/>
<connect gate="A" pin="DS" pad="19"/>
<connect gate="A" pin="E/QE" pad="5"/>
<connect gate="A" pin="F/QF" pad="6"/>
<connect gate="A" pin="G" pad="16"/>
<connect gate="A" pin="G/QG" pad="7"/>
<connect gate="A" pin="H/QH" pad="8"/>
<connect gate="A" pin="QH*" pad="11"/>
<connect gate="A" pin="RCK" pad="15"/>
<connect gate="A" pin="SCK" pad="13"/>
<connect gate="A" pin="SCKE" pad="14"/>
<connect gate="A" pin="SCL" pad="12"/>
<connect gate="A" pin="SLD" pad="9"/>
<connect gate="A" pin="SR0" pad="18"/>
<connect gate="A" pin="SR1" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*599" prefix="IC">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch, open collector</description>
<gates>
<gate name="A" symbol="74599"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="RCL" pad="13"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="QA" pad="15"/>
<connect gate="A" pin="QB" pad="1"/>
<connect gate="A" pin="QC" pad="2"/>
<connect gate="A" pin="QD" pad="3"/>
<connect gate="A" pin="QE" pad="4"/>
<connect gate="A" pin="QF" pad="5"/>
<connect gate="A" pin="QG" pad="6"/>
<connect gate="A" pin="QH" pad="7"/>
<connect gate="A" pin="QH*" pad="9"/>
<connect gate="A" pin="RCK" pad="12"/>
<connect gate="A" pin="RCL" pad="13"/>
<connect gate="A" pin="SCK" pad="11"/>
<connect gate="A" pin="SCL" pad="10"/>
<connect gate="A" pin="SER" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*604" prefix="IC">
<description>Octal 2-input &lt;b&gt;MULTIPLEXED LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74604"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL28-6">
<connects>
<connect gate="A" pin="A/!B" pad="2"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="7"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="27"/>
<connect gate="A" pin="A6" pad="25"/>
<connect gate="A" pin="A7" pad="23"/>
<connect gate="A" pin="A8" pad="21"/>
<connect gate="A" pin="B1" pad="4"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="B3" pad="8"/>
<connect gate="A" pin="B4" pad="10"/>
<connect gate="A" pin="B5" pad="26"/>
<connect gate="A" pin="B6" pad="24"/>
<connect gate="A" pin="B7" pad="22"/>
<connect gate="A" pin="B8" pad="20"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="Y1" pad="15"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="16"/>
<connect gate="A" pin="Y6" pad="17"/>
<connect gate="A" pin="Y7" pad="18"/>
<connect gate="A" pin="Y8" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*605" prefix="IC">
<description>Octal 2-input &lt;b&gt;MULTIPLEXED LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74605"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL28-6">
<connects>
<connect gate="A" pin="A/!B" pad="2"/>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="7"/>
<connect gate="A" pin="A4" pad="9"/>
<connect gate="A" pin="A5" pad="27"/>
<connect gate="A" pin="A6" pad="25"/>
<connect gate="A" pin="A7" pad="23"/>
<connect gate="A" pin="A8" pad="21"/>
<connect gate="A" pin="B1" pad="4"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="B3" pad="8"/>
<connect gate="A" pin="B4" pad="10"/>
<connect gate="A" pin="B5" pad="26"/>
<connect gate="A" pin="B6" pad="24"/>
<connect gate="A" pin="B7" pad="22"/>
<connect gate="A" pin="B8" pad="20"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="Y1" pad="15"/>
<connect gate="A" pin="Y2" pad="13"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="16"/>
<connect gate="A" pin="Y6" pad="17"/>
<connect gate="A" pin="Y7" pad="18"/>
<connect gate="A" pin="Y8" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*608" prefix="IC">
<description>&lt;b&gt;MEMORY CYCLE CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74608"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!CAS" pad="9"/>
<connect gate="A" pin="!RAS" pad="7"/>
<connect gate="A" pin="CAS/!HLD" pad="10"/>
<connect gate="A" pin="P/!N" pad="2"/>
<connect gate="A" pin="PRECHRG" pad="1"/>
<connect gate="A" pin="R/!W_I" pad="3"/>
<connect gate="A" pin="R/!W_O" pad="5"/>
<connect gate="A" pin="RAS_EN" pad="6"/>
<connect gate="A" pin="RC/CAS" pad="15"/>
<connect gate="A" pin="RC_RAH" pad="12"/>
<connect gate="A" pin="REFRESH" pad="14"/>
<connect gate="A" pin="RMW" pad="4"/>
<connect gate="A" pin="ROW/!COL" pad="11"/>
<connect gate="A" pin="START" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*620" prefix="IC">
<description>Octal &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74620"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="GAB" pad="1"/>
<connect gate="A" pin="GBA" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*621" prefix="IC">
<description>Octal &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="74621"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="B1" pad="18"/>
<connect gate="A" pin="B2" pad="17"/>
<connect gate="A" pin="B3" pad="16"/>
<connect gate="A" pin="B4" pad="15"/>
<connect gate="A" pin="B5" pad="14"/>
<connect gate="A" pin="B6" pad="13"/>
<connect gate="A" pin="B7" pad="12"/>
<connect gate="A" pin="B8" pad="11"/>
<connect gate="A" pin="GAB" pad="1"/>
<connect gate="A" pin="GBA" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*651" prefix="IC">
<description>8-bit &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt; and &lt;b&gt;REGISTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74651"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="7"/>
<connect gate="A" pin="A5" pad="8"/>
<connect gate="A" pin="A6" pad="9"/>
<connect gate="A" pin="A7" pad="10"/>
<connect gate="A" pin="A8" pad="11"/>
<connect gate="A" pin="B1" pad="20"/>
<connect gate="A" pin="B2" pad="19"/>
<connect gate="A" pin="B3" pad="18"/>
<connect gate="A" pin="B4" pad="17"/>
<connect gate="A" pin="B5" pad="16"/>
<connect gate="A" pin="B6" pad="15"/>
<connect gate="A" pin="B7" pad="14"/>
<connect gate="A" pin="B8" pad="13"/>
<connect gate="A" pin="CAB" pad="1"/>
<connect gate="A" pin="CBA" pad="23"/>
<connect gate="A" pin="GAB" pad="3"/>
<connect gate="A" pin="GBA" pad="21"/>
<connect gate="A" pin="SAB" pad="2"/>
<connect gate="A" pin="SBA" pad="22"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*668" prefix="IC">
<description>4-bit synchronous decade &lt;b&gt;COUNTER&lt;/b&gt;, preset</description>
<gates>
<gate name="A" symbol="74668"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="10"/>
<connect gate="A" pin="LD" pad="9"/>
<connect gate="A" pin="QA" pad="14"/>
<connect gate="A" pin="QB" pad="13"/>
<connect gate="A" pin="QC" pad="12"/>
<connect gate="A" pin="QD" pad="11"/>
<connect gate="A" pin="RCO" pad="15"/>
<connect gate="A" pin="U/!D" pad="1"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*670" prefix="IC">
<description>4 by 4 &lt;b&gt;REGISTER FILES&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74670"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D2" pad="1"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="3"/>
<connect gate="A" pin="GR" pad="11"/>
<connect gate="A" pin="GW" pad="12"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="6"/>
<connect gate="A" pin="RA" pad="5"/>
<connect gate="A" pin="RB" pad="4"/>
<connect gate="A" pin="WA" pad="14"/>
<connect gate="A" pin="WB" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D1" pad="15"/>
<connect gate="A" pin="D2" pad="1"/>
<connect gate="A" pin="D3" pad="2"/>
<connect gate="A" pin="D4" pad="3"/>
<connect gate="A" pin="GR" pad="11"/>
<connect gate="A" pin="GW" pad="12"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="7"/>
<connect gate="A" pin="Q4" pad="6"/>
<connect gate="A" pin="RA" pad="5"/>
<connect gate="A" pin="RB" pad="4"/>
<connect gate="A" pin="WA" pad="14"/>
<connect gate="A" pin="WB" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="D1" pad="19"/>
<connect gate="A" pin="D2" pad="2"/>
<connect gate="A" pin="D3" pad="3"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="GR" pad="14"/>
<connect gate="A" pin="GW" pad="15"/>
<connect gate="A" pin="Q1" pad="13"/>
<connect gate="A" pin="Q2" pad="12"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="8"/>
<connect gate="A" pin="RA" pad="7"/>
<connect gate="A" pin="RB" pad="5"/>
<connect gate="A" pin="WA" pad="18"/>
<connect gate="A" pin="WB" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*671" prefix="IC">
<description>4-bit universal &lt;b&gt;SHIFT REGISTER/LATCH&lt;/b&gt;, 3-state</description>
<gates>
<gate name="A" symbol="74671"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CASC" pad="19"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="QA" pad="18"/>
<connect gate="A" pin="QB" pad="17"/>
<connect gate="A" pin="QC" pad="16"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="R/!S" pad="11"/>
<connect gate="A" pin="RCK" pad="9"/>
<connect gate="A" pin="S0" pad="14"/>
<connect gate="A" pin="S1" pad="13"/>
<connect gate="A" pin="SCK" pad="2"/>
<connect gate="A" pin="SCL" pad="8"/>
<connect gate="A" pin="SRL" pad="7"/>
<connect gate="A" pin="SRR" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*673" prefix="IC">
<description>16-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt; serial to parallel conversion</description>
<gates>
<gate name="A" symbol="74673"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="M/SCLK" pad="5"/>
<connect gate="A" pin="R/!W" pad="3"/>
<connect gate="A" pin="SER/Q15" pad="6"/>
<connect gate="A" pin="SHCLK" pad="2"/>
<connect gate="A" pin="STRCLR" pad="4"/>
<connect gate="A" pin="Y0" pad="7"/>
<connect gate="A" pin="Y1" pad="8"/>
<connect gate="A" pin="Y10" pad="18"/>
<connect gate="A" pin="Y11" pad="19"/>
<connect gate="A" pin="Y12" pad="20"/>
<connect gate="A" pin="Y13" pad="21"/>
<connect gate="A" pin="Y14" pad="22"/>
<connect gate="A" pin="Y15" pad="23"/>
<connect gate="A" pin="Y2" pad="9"/>
<connect gate="A" pin="Y3" pad="10"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="13"/>
<connect gate="A" pin="Y6" pad="14"/>
<connect gate="A" pin="Y7" pad="15"/>
<connect gate="A" pin="Y8" pad="16"/>
<connect gate="A" pin="Y9" pad="17"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO24W">
<connects>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="M/SCLK" pad="5"/>
<connect gate="A" pin="R/!W" pad="3"/>
<connect gate="A" pin="SER/Q15" pad="6"/>
<connect gate="A" pin="SHCLK" pad="2"/>
<connect gate="A" pin="STRCLR" pad="4"/>
<connect gate="A" pin="Y0" pad="7"/>
<connect gate="A" pin="Y1" pad="8"/>
<connect gate="A" pin="Y10" pad="18"/>
<connect gate="A" pin="Y11" pad="19"/>
<connect gate="A" pin="Y12" pad="20"/>
<connect gate="A" pin="Y13" pad="21"/>
<connect gate="A" pin="Y14" pad="22"/>
<connect gate="A" pin="Y15" pad="23"/>
<connect gate="A" pin="Y2" pad="9"/>
<connect gate="A" pin="Y3" pad="10"/>
<connect gate="A" pin="Y4" pad="11"/>
<connect gate="A" pin="Y5" pad="13"/>
<connect gate="A" pin="Y6" pad="14"/>
<connect gate="A" pin="Y7" pad="15"/>
<connect gate="A" pin="Y8" pad="16"/>
<connect gate="A" pin="Y9" pad="17"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC28">
<connects>
<connect gate="A" pin="CS" pad="2"/>
<connect gate="A" pin="M/SCLK" pad="6"/>
<connect gate="A" pin="R/!W" pad="4"/>
<connect gate="A" pin="SER/Q15" pad="7"/>
<connect gate="A" pin="SHCLK" pad="3"/>
<connect gate="A" pin="STRCLR" pad="5"/>
<connect gate="A" pin="Y0" pad="9"/>
<connect gate="A" pin="Y1" pad="10"/>
<connect gate="A" pin="Y10" pad="21"/>
<connect gate="A" pin="Y11" pad="23"/>
<connect gate="A" pin="Y12" pad="24"/>
<connect gate="A" pin="Y13" pad="25"/>
<connect gate="A" pin="Y14" pad="26"/>
<connect gate="A" pin="Y15" pad="27"/>
<connect gate="A" pin="Y2" pad="11"/>
<connect gate="A" pin="Y3" pad="12"/>
<connect gate="A" pin="Y4" pad="13"/>
<connect gate="A" pin="Y5" pad="16"/>
<connect gate="A" pin="Y6" pad="17"/>
<connect gate="A" pin="Y7" pad="18"/>
<connect gate="A" pin="Y8" pad="19"/>
<connect gate="A" pin="Y9" pad="20"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*674" prefix="IC">
<description>16-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt; parallel to serial conversion</description>
<gates>
<gate name="A" symbol="74674"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="MOD" pad="5"/>
<connect gate="A" pin="P0" pad="7"/>
<connect gate="A" pin="P1" pad="8"/>
<connect gate="A" pin="P10" pad="18"/>
<connect gate="A" pin="P11" pad="19"/>
<connect gate="A" pin="P12" pad="20"/>
<connect gate="A" pin="P13" pad="21"/>
<connect gate="A" pin="P14" pad="22"/>
<connect gate="A" pin="P15" pad="23"/>
<connect gate="A" pin="P2" pad="9"/>
<connect gate="A" pin="P3" pad="10"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="14"/>
<connect gate="A" pin="P7" pad="15"/>
<connect gate="A" pin="P8" pad="16"/>
<connect gate="A" pin="P9" pad="17"/>
<connect gate="A" pin="R/!W" pad="3"/>
<connect gate="A" pin="SER/Q15" pad="6"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO24W">
<connects>
<connect gate="A" pin="CLK" pad="2"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="MOD" pad="5"/>
<connect gate="A" pin="P0" pad="7"/>
<connect gate="A" pin="P1" pad="8"/>
<connect gate="A" pin="P10" pad="18"/>
<connect gate="A" pin="P11" pad="19"/>
<connect gate="A" pin="P12" pad="20"/>
<connect gate="A" pin="P13" pad="21"/>
<connect gate="A" pin="P14" pad="22"/>
<connect gate="A" pin="P15" pad="23"/>
<connect gate="A" pin="P2" pad="9"/>
<connect gate="A" pin="P3" pad="10"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="14"/>
<connect gate="A" pin="P7" pad="15"/>
<connect gate="A" pin="P8" pad="16"/>
<connect gate="A" pin="P9" pad="17"/>
<connect gate="A" pin="R/!W" pad="3"/>
<connect gate="A" pin="SER/Q15" pad="6"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC28">
<connects>
<connect gate="A" pin="CLK" pad="3"/>
<connect gate="A" pin="CS" pad="2"/>
<connect gate="A" pin="MOD" pad="6"/>
<connect gate="A" pin="P0" pad="9"/>
<connect gate="A" pin="P1" pad="10"/>
<connect gate="A" pin="P10" pad="21"/>
<connect gate="A" pin="P11" pad="23"/>
<connect gate="A" pin="P12" pad="24"/>
<connect gate="A" pin="P13" pad="25"/>
<connect gate="A" pin="P14" pad="26"/>
<connect gate="A" pin="P15" pad="27"/>
<connect gate="A" pin="P2" pad="11"/>
<connect gate="A" pin="P3" pad="12"/>
<connect gate="A" pin="P4" pad="13"/>
<connect gate="A" pin="P5" pad="16"/>
<connect gate="A" pin="P6" pad="17"/>
<connect gate="A" pin="P7" pad="18"/>
<connect gate="A" pin="P8" pad="19"/>
<connect gate="A" pin="P9" pad="20"/>
<connect gate="A" pin="R/!W" pad="4"/>
<connect gate="A" pin="SER/Q15" pad="7"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*678" prefix="IC">
<description>16-bit address &lt;b&gt;COMPARATOR&lt;/b&gt;, latch</description>
<gates>
<gate name="A" symbol="74678"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A10" pad="10"/>
<connect gate="A" pin="A11" pad="11"/>
<connect gate="A" pin="A12" pad="13"/>
<connect gate="A" pin="A13" pad="14"/>
<connect gate="A" pin="A14" pad="15"/>
<connect gate="A" pin="A15" pad="16"/>
<connect gate="A" pin="A16" pad="17"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="6"/>
<connect gate="A" pin="A7" pad="7"/>
<connect gate="A" pin="A8" pad="8"/>
<connect gate="A" pin="A9" pad="9"/>
<connect gate="A" pin="G" pad="23"/>
<connect gate="A" pin="P0" pad="18"/>
<connect gate="A" pin="P1" pad="19"/>
<connect gate="A" pin="P2" pad="20"/>
<connect gate="A" pin="P3" pad="21"/>
<connect gate="A" pin="Y" pad="22"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*679" prefix="IC">
<description>12-bit address &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74679"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A10" pad="11"/>
<connect gate="A" pin="A11" pad="12"/>
<connect gate="A" pin="A12" pad="13"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="6"/>
<connect gate="A" pin="A7" pad="7"/>
<connect gate="A" pin="A8" pad="8"/>
<connect gate="A" pin="A9" pad="9"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="A" pin="P0" pad="14"/>
<connect gate="A" pin="P1" pad="15"/>
<connect gate="A" pin="P2" pad="16"/>
<connect gate="A" pin="P3" pad="17"/>
<connect gate="A" pin="Y" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*680" prefix="IC">
<description>12-bit address &lt;b&gt;COMPARATOR&lt;/b&gt;, latch</description>
<gates>
<gate name="A" symbol="74680"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="1"/>
<connect gate="A" pin="A10" pad="11"/>
<connect gate="A" pin="A11" pad="12"/>
<connect gate="A" pin="A12" pad="13"/>
<connect gate="A" pin="A2" pad="2"/>
<connect gate="A" pin="A3" pad="3"/>
<connect gate="A" pin="A4" pad="4"/>
<connect gate="A" pin="A5" pad="5"/>
<connect gate="A" pin="A6" pad="6"/>
<connect gate="A" pin="A7" pad="7"/>
<connect gate="A" pin="A8" pad="8"/>
<connect gate="A" pin="A9" pad="9"/>
<connect gate="A" pin="G" pad="19"/>
<connect gate="A" pin="P0" pad="14"/>
<connect gate="A" pin="P1" pad="15"/>
<connect gate="A" pin="P2" pad="16"/>
<connect gate="A" pin="P3" pad="17"/>
<connect gate="A" pin="Y" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*681" prefix="IC">
<description>4-bit parallel binary &lt;b&gt;ACCUMULATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74681"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="AS0" pad="18"/>
<connect gate="A" pin="AS1" pad="17"/>
<connect gate="A" pin="AS2" pad="16"/>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="CN" pad="6"/>
<connect gate="A" pin="CN+4" pad="8"/>
<connect gate="A" pin="G" pad="7"/>
<connect gate="A" pin="I/O0" pad="14"/>
<connect gate="A" pin="I/O1" pad="13"/>
<connect gate="A" pin="I/O2" pad="12"/>
<connect gate="A" pin="I/O3" pad="11"/>
<connect gate="A" pin="LI/RO" pad="5"/>
<connect gate="A" pin="MOD" pad="15"/>
<connect gate="A" pin="P" pad="9"/>
<connect gate="A" pin="RI/LO" pad="19"/>
<connect gate="A" pin="RS0" pad="4"/>
<connect gate="A" pin="RS1" pad="3"/>
<connect gate="A" pin="RS2" pad="2"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*682" prefix="IC">
<description>8-bit &lt;b&gt;MAGNITUDE/IDENTITY COMPARATOR&lt;/b&gt;, totem pole</description>
<gates>
<gate name="A" symbol="74682"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="P&gt;Q" pad="1"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="P&gt;Q" pad="1"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="P&gt;Q" pad="1"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*683" prefix="IC">
<description>8-bit &lt;b&gt;MAGNITUDE/IDENTITY COMPARATOR&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="74683"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="P&gt;Q" pad="1"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*686" prefix="IC">
<description>8-bit &lt;b&gt;MAGNITUDE/IDENTITY COMPARATOR&lt;/b&gt;, totem pole</description>
<gates>
<gate name="A" symbol="74686"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="23"/>
<connect gate="A" pin="P0" pad="3"/>
<connect gate="A" pin="P1" pad="5"/>
<connect gate="A" pin="P2" pad="8"/>
<connect gate="A" pin="P3" pad="10"/>
<connect gate="A" pin="P4" pad="13"/>
<connect gate="A" pin="P5" pad="15"/>
<connect gate="A" pin="P6" pad="17"/>
<connect gate="A" pin="P7" pad="20"/>
<connect gate="A" pin="P=Q" pad="22"/>
<connect gate="A" pin="P&gt;Q" pad="1"/>
<connect gate="A" pin="Q0" pad="4"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="11"/>
<connect gate="A" pin="Q4" pad="14"/>
<connect gate="A" pin="Q5" pad="16"/>
<connect gate="A" pin="Q6" pad="18"/>
<connect gate="A" pin="Q7" pad="21"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO24W">
<connects>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="23"/>
<connect gate="A" pin="P0" pad="3"/>
<connect gate="A" pin="P1" pad="5"/>
<connect gate="A" pin="P2" pad="8"/>
<connect gate="A" pin="P3" pad="10"/>
<connect gate="A" pin="P4" pad="13"/>
<connect gate="A" pin="P5" pad="15"/>
<connect gate="A" pin="P6" pad="17"/>
<connect gate="A" pin="P7" pad="20"/>
<connect gate="A" pin="P=Q" pad="22"/>
<connect gate="A" pin="P&gt;Q" pad="1"/>
<connect gate="A" pin="Q0" pad="4"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="11"/>
<connect gate="A" pin="Q4" pad="14"/>
<connect gate="A" pin="Q5" pad="16"/>
<connect gate="A" pin="Q6" pad="18"/>
<connect gate="A" pin="Q7" pad="21"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC28">
<connects>
<connect gate="A" pin="G1" pad="3"/>
<connect gate="A" pin="G2" pad="27"/>
<connect gate="A" pin="P0" pad="4"/>
<connect gate="A" pin="P1" pad="6"/>
<connect gate="A" pin="P2" pad="10"/>
<connect gate="A" pin="P3" pad="12"/>
<connect gate="A" pin="P4" pad="16"/>
<connect gate="A" pin="P5" pad="18"/>
<connect gate="A" pin="P6" pad="20"/>
<connect gate="A" pin="P7" pad="24"/>
<connect gate="A" pin="P=Q" pad="26"/>
<connect gate="A" pin="P&gt;Q" pad="2"/>
<connect gate="A" pin="Q0" pad="5"/>
<connect gate="A" pin="Q1" pad="7"/>
<connect gate="A" pin="Q2" pad="11"/>
<connect gate="A" pin="Q3" pad="13"/>
<connect gate="A" pin="Q4" pad="17"/>
<connect gate="A" pin="Q5" pad="19"/>
<connect gate="A" pin="Q6" pad="21"/>
<connect gate="A" pin="Q7" pad="25"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*687" prefix="IC">
<description>8-bit &lt;b&gt;MAGNITUDE/IDENTITY COMPARATOR&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="74687"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="G1" pad="2"/>
<connect gate="A" pin="G2" pad="23"/>
<connect gate="A" pin="P0" pad="3"/>
<connect gate="A" pin="P1" pad="5"/>
<connect gate="A" pin="P2" pad="8"/>
<connect gate="A" pin="P3" pad="10"/>
<connect gate="A" pin="P4" pad="13"/>
<connect gate="A" pin="P5" pad="15"/>
<connect gate="A" pin="P6" pad="17"/>
<connect gate="A" pin="P7" pad="20"/>
<connect gate="A" pin="P=Q" pad="22"/>
<connect gate="A" pin="P&gt;Q" pad="1"/>
<connect gate="A" pin="Q0" pad="4"/>
<connect gate="A" pin="Q1" pad="6"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="11"/>
<connect gate="A" pin="Q4" pad="14"/>
<connect gate="A" pin="Q5" pad="16"/>
<connect gate="A" pin="Q6" pad="18"/>
<connect gate="A" pin="Q7" pad="21"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*688" prefix="IC">
<description>8-bit &lt;b&gt;MAGNITUDE/IDENTITY COMPARATOR&lt;/b&gt;, totem pole</description>
<gates>
<gate name="A" symbol="74688"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*689" prefix="IC">
<description>8-bit &lt;b&gt;MAGNITUDE/IDENTITY COMPARATOR&lt;/b&gt;, open collector</description>
<gates>
<gate name="A" symbol="74689"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="P0" pad="2"/>
<connect gate="A" pin="P1" pad="4"/>
<connect gate="A" pin="P2" pad="6"/>
<connect gate="A" pin="P3" pad="8"/>
<connect gate="A" pin="P4" pad="11"/>
<connect gate="A" pin="P5" pad="13"/>
<connect gate="A" pin="P6" pad="15"/>
<connect gate="A" pin="P7" pad="17"/>
<connect gate="A" pin="P=Q" pad="19"/>
<connect gate="A" pin="Q0" pad="3"/>
<connect gate="A" pin="Q1" pad="5"/>
<connect gate="A" pin="Q2" pad="7"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="12"/>
<connect gate="A" pin="Q5" pad="14"/>
<connect gate="A" pin="Q6" pad="16"/>
<connect gate="A" pin="Q7" pad="18"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*690" prefix="IC">
<description>Synchronous &lt;b&gt;DECADE COUNTER&lt;/b&gt;, register, 3-state</description>
<gates>
<gate name="A" symbol="74690"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CCK" pad="2"/>
<connect gate="A" pin="CCL" pad="1"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="14"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="LD" pad="13"/>
<connect gate="A" pin="QA" pad="18"/>
<connect gate="A" pin="QB" pad="17"/>
<connect gate="A" pin="QC" pad="16"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="R/!C" pad="11"/>
<connect gate="A" pin="RCK" pad="9"/>
<connect gate="A" pin="RCL" pad="8"/>
<connect gate="A" pin="RCO" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*696" prefix="IC">
<description>Synchronous decade &lt;b&gt;UP/DOWN COUNTER&lt;/b&gt;, register, 3-state</description>
<gates>
<gate name="A" symbol="74696"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CCK" pad="2"/>
<connect gate="A" pin="CCL" pad="8"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="14"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="LD" pad="13"/>
<connect gate="A" pin="QA" pad="18"/>
<connect gate="A" pin="QB" pad="17"/>
<connect gate="A" pin="QC" pad="16"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="R/!C" pad="11"/>
<connect gate="A" pin="RCK" pad="9"/>
<connect gate="A" pin="RCO" pad="19"/>
<connect gate="A" pin="U/!D" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*746" prefix="IC">
<description>Octal &lt;b&gt;BUS DRIVER&lt;/b&gt;, inverting, pull-up resistors</description>
<gates>
<gate name="A" symbol="74746"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*747" prefix="IC">
<description>Octal &lt;b&gt;BUS DRIVER&lt;/b&gt;, true, pull-up resistors</description>
<gates>
<gate name="A" symbol="74747"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="3"/>
<connect gate="A" pin="A3" pad="4"/>
<connect gate="A" pin="A4" pad="5"/>
<connect gate="A" pin="A5" pad="6"/>
<connect gate="A" pin="A6" pad="7"/>
<connect gate="A" pin="A7" pad="8"/>
<connect gate="A" pin="A8" pad="9"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="19"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="17"/>
<connect gate="A" pin="Y3" pad="16"/>
<connect gate="A" pin="Y4" pad="15"/>
<connect gate="A" pin="Y5" pad="14"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="A" pin="Y7" pad="12"/>
<connect gate="A" pin="Y8" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*756" prefix="IC">
<description>8-bit inverting &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74756"/>
<gate name="B" symbol="74756"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*762" prefix="IC">
<description>8-bit &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74762"/>
<gate name="B" symbol="74762"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*763" prefix="IC">
<description>8-bit inverting &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74763"/>
<gate name="B" symbol="74763"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G1" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*804" prefix="IC">
<description>Hex &lt;b&gt;NAND&lt;/b&gt; driver</description>
<gates>
<gate name="A" symbol="74804"/>
<gate name="B" symbol="74804"/>
<gate name="C" symbol="74804"/>
<gate name="D" symbol="74804"/>
<gate name="E" symbol="74804"/>
<gate name="F" symbol="74804"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="7"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="E" pin="I0" pad="15"/>
<connect gate="E" pin="I1" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I0" pad="18"/>
<connect gate="F" pin="I1" pad="19"/>
<connect gate="F" pin="O" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*805" prefix="IC">
<description>Hex &lt;b&gt;NOR&lt;/b&gt; driver</description>
<gates>
<gate name="A" symbol="74805"/>
<gate name="B" symbol="74805"/>
<gate name="C" symbol="74805"/>
<gate name="D" symbol="74805"/>
<gate name="E" symbol="74805"/>
<gate name="F" symbol="74805"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="7"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="E" pin="I0" pad="15"/>
<connect gate="E" pin="I1" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I0" pad="18"/>
<connect gate="F" pin="I1" pad="19"/>
<connect gate="F" pin="O" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*808" prefix="IC">
<description>Hex &lt;b&gt;AND&lt;/b&gt; driver</description>
<gates>
<gate name="A" symbol="74808"/>
<gate name="B" symbol="74808"/>
<gate name="C" symbol="74808"/>
<gate name="D" symbol="74808"/>
<gate name="E" symbol="74808"/>
<gate name="F" symbol="74808"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="7"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="E" pin="I0" pad="15"/>
<connect gate="E" pin="I1" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I0" pad="18"/>
<connect gate="F" pin="I1" pad="19"/>
<connect gate="F" pin="O" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*811" prefix="IC">
<description>Quad &lt;b&gt;EX-NOR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="74811"/>
<gate name="B" symbol="74811"/>
<gate name="C" symbol="74811"/>
<gate name="D" symbol="74811"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*832" prefix="IC">
<description>Hex &lt;b&gt;OR&lt;/b&gt; driver</description>
<gates>
<gate name="A" symbol="74832"/>
<gate name="B" symbol="74832"/>
<gate name="C" symbol="74832"/>
<gate name="D" symbol="74832"/>
<gate name="E" symbol="74832"/>
<gate name="F" symbol="74832"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="7"/>
<connect gate="C" pin="I1" pad="8"/>
<connect gate="C" pin="O" pad="9"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="E" pin="I0" pad="15"/>
<connect gate="E" pin="I1" pad="16"/>
<connect gate="E" pin="O" pad="14"/>
<connect gate="F" pin="I0" pad="18"/>
<connect gate="F" pin="I1" pad="19"/>
<connect gate="F" pin="O" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*850" prefix="IC">
<description>16-to 1 line &lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74850"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL28-6">
<connects>
<connect gate="A" pin="CLK" pad="12"/>
<connect gate="A" pin="D0" pad="8"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D10" pad="25"/>
<connect gate="A" pin="D11" pad="24"/>
<connect gate="A" pin="D12" pad="23"/>
<connect gate="A" pin="D13" pad="22"/>
<connect gate="A" pin="D14" pad="21"/>
<connect gate="A" pin="D15" pad="20"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="D5" pad="3"/>
<connect gate="A" pin="D6" pad="2"/>
<connect gate="A" pin="D7" pad="1"/>
<connect gate="A" pin="D8" pad="27"/>
<connect gate="A" pin="D9" pad="26"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="A" pin="GW" pad="11"/>
<connect gate="A" pin="GY" pad="9"/>
<connect gate="A" pin="S0" pad="18"/>
<connect gate="A" pin="S1" pad="17"/>
<connect gate="A" pin="S2" pad="16"/>
<connect gate="A" pin="S3" pad="15"/>
<connect gate="A" pin="W" pad="13"/>
<connect gate="A" pin="Y" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*851" prefix="IC">
<description>16-to 1 line &lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74851"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL28-6">
<connects>
<connect gate="A" pin="D0" pad="8"/>
<connect gate="A" pin="D1" pad="7"/>
<connect gate="A" pin="D10" pad="25"/>
<connect gate="A" pin="D11" pad="24"/>
<connect gate="A" pin="D12" pad="23"/>
<connect gate="A" pin="D13" pad="22"/>
<connect gate="A" pin="D14" pad="21"/>
<connect gate="A" pin="D15" pad="20"/>
<connect gate="A" pin="D2" pad="6"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="4"/>
<connect gate="A" pin="D5" pad="3"/>
<connect gate="A" pin="D6" pad="2"/>
<connect gate="A" pin="D7" pad="1"/>
<connect gate="A" pin="D8" pad="27"/>
<connect gate="A" pin="D9" pad="26"/>
<connect gate="A" pin="G" pad="10"/>
<connect gate="A" pin="GW" pad="11"/>
<connect gate="A" pin="GY" pad="9"/>
<connect gate="A" pin="S0" pad="18"/>
<connect gate="A" pin="S1" pad="17"/>
<connect gate="A" pin="S2" pad="16"/>
<connect gate="A" pin="S3" pad="15"/>
<connect gate="A" pin="SC" pad="12"/>
<connect gate="A" pin="W" pad="13"/>
<connect gate="A" pin="Y" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*852" prefix="IC">
<description>8-bit bidirectional &lt;b&gt;DRIVER&lt;/b&gt; and &lt;b&gt;PORT CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74852"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="7"/>
<connect gate="A" pin="A5" pad="8"/>
<connect gate="A" pin="A6" pad="9"/>
<connect gate="A" pin="A7" pad="10"/>
<connect gate="A" pin="A8" pad="11"/>
<connect gate="A" pin="B1" pad="21"/>
<connect gate="A" pin="B2" pad="20"/>
<connect gate="A" pin="B3" pad="19"/>
<connect gate="A" pin="B4" pad="18"/>
<connect gate="A" pin="B5" pad="17"/>
<connect gate="A" pin="B6" pad="16"/>
<connect gate="A" pin="B7" pad="15"/>
<connect gate="A" pin="B8" pad="14"/>
<connect gate="A" pin="CLK" pad="23"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="A" pin="SRI" pad="22"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*856" prefix="IC">
<description>8-bit bidirectional &lt;b&gt;DRIVER&lt;/b&gt; and &lt;b&gt;PORT CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74856"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="7"/>
<connect gate="A" pin="A5" pad="8"/>
<connect gate="A" pin="A6" pad="9"/>
<connect gate="A" pin="A7" pad="10"/>
<connect gate="A" pin="A8" pad="11"/>
<connect gate="A" pin="B1" pad="21"/>
<connect gate="A" pin="B2" pad="20"/>
<connect gate="A" pin="B3" pad="19"/>
<connect gate="A" pin="B4" pad="18"/>
<connect gate="A" pin="B5" pad="17"/>
<connect gate="A" pin="B6" pad="16"/>
<connect gate="A" pin="B7" pad="15"/>
<connect gate="A" pin="B8" pad="14"/>
<connect gate="A" pin="CLK" pad="23"/>
<connect gate="A" pin="MOD" pad="3"/>
<connect gate="A" pin="OEA" pad="2"/>
<connect gate="A" pin="OEB" pad="1"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="SRI" pad="22"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*857" prefix="IC">
<description>Hex 2-to 1 line universal &lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74857"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="1A" pad="2"/>
<connect gate="A" pin="1B" pad="3"/>
<connect gate="A" pin="1Y" pad="4"/>
<connect gate="A" pin="2A" pad="5"/>
<connect gate="A" pin="2B" pad="6"/>
<connect gate="A" pin="2Y" pad="7"/>
<connect gate="A" pin="3A" pad="8"/>
<connect gate="A" pin="3B" pad="9"/>
<connect gate="A" pin="3Y" pad="10"/>
<connect gate="A" pin="4A" pad="16"/>
<connect gate="A" pin="4B" pad="15"/>
<connect gate="A" pin="4Y" pad="14"/>
<connect gate="A" pin="5A" pad="19"/>
<connect gate="A" pin="5B" pad="18"/>
<connect gate="A" pin="5Y" pad="17"/>
<connect gate="A" pin="6A" pad="22"/>
<connect gate="A" pin="6B" pad="21"/>
<connect gate="A" pin="6Y" pad="20"/>
<connect gate="A" pin="CMP" pad="13"/>
<connect gate="A" pin="O=0" pad="11"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="23"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*866" prefix="IC">
<description>8-bit magnitude &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74866"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL28-6">
<connects>
<connect gate="A" pin="CLRQ" pad="27"/>
<connect gate="A" pin="L/!A" pad="2"/>
<connect gate="A" pin="OLE" pad="15"/>
<connect gate="A" pin="P0" pad="18"/>
<connect gate="A" pin="P1" pad="19"/>
<connect gate="A" pin="P2" pad="20"/>
<connect gate="A" pin="P3" pad="21"/>
<connect gate="A" pin="P4" pad="22"/>
<connect gate="A" pin="P5" pad="23"/>
<connect gate="A" pin="P6" pad="24"/>
<connect gate="A" pin="P7" pad="25"/>
<connect gate="A" pin="P&lt;Q_0" pad="17"/>
<connect gate="A" pin="P&lt;Q_I" pad="3"/>
<connect gate="A" pin="P=Q_O" pad="13"/>
<connect gate="A" pin="P&gt;Q_I" pad="4"/>
<connect gate="A" pin="P&gt;Q_O" pad="16"/>
<connect gate="A" pin="PLE" pad="26"/>
<connect gate="A" pin="Q0" pad="12"/>
<connect gate="A" pin="Q1" pad="11"/>
<connect gate="A" pin="Q2" pad="10"/>
<connect gate="A" pin="Q3" pad="9"/>
<connect gate="A" pin="Q4" pad="8"/>
<connect gate="A" pin="Q5" pad="7"/>
<connect gate="A" pin="Q6" pad="6"/>
<connect gate="A" pin="Q7" pad="5"/>
<connect gate="A" pin="QLE" pad="1"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*867" prefix="IC">
<description>8-bit synchronous &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74867"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="E" pad="7"/>
<connect gate="A" pin="ENP" pad="23"/>
<connect gate="A" pin="ENT" pad="11"/>
<connect gate="A" pin="F" pad="8"/>
<connect gate="A" pin="G" pad="9"/>
<connect gate="A" pin="H" pad="10"/>
<connect gate="A" pin="QA" pad="22"/>
<connect gate="A" pin="QB" pad="21"/>
<connect gate="A" pin="QC" pad="20"/>
<connect gate="A" pin="QD" pad="19"/>
<connect gate="A" pin="QE" pad="18"/>
<connect gate="A" pin="QF" pad="17"/>
<connect gate="A" pin="QG" pad="16"/>
<connect gate="A" pin="QH" pad="15"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*873" prefix="IC">
<description>2 x 4-bit &lt;b&gt;D type LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74873"/>
<gate name="B" symbol="74873"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="C" pad="23"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="OC" pad="2"/>
<connect gate="A" pin="Q1" pad="22"/>
<connect gate="A" pin="Q2" pad="21"/>
<connect gate="A" pin="Q3" pad="20"/>
<connect gate="A" pin="Q4" pad="19"/>
<connect gate="B" pin="C" pad="14"/>
<connect gate="B" pin="CLR" pad="13"/>
<connect gate="B" pin="D1" pad="7"/>
<connect gate="B" pin="D2" pad="8"/>
<connect gate="B" pin="D3" pad="9"/>
<connect gate="B" pin="D4" pad="10"/>
<connect gate="B" pin="OC" pad="11"/>
<connect gate="B" pin="Q1" pad="18"/>
<connect gate="B" pin="Q2" pad="17"/>
<connect gate="B" pin="Q3" pad="16"/>
<connect gate="B" pin="Q4" pad="15"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*874" prefix="IC">
<description>2 x 4-bit &lt;b&gt;D type FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74874"/>
<gate name="B" symbol="74874"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="CLK" pad="23"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="OC" pad="2"/>
<connect gate="A" pin="Q1" pad="22"/>
<connect gate="A" pin="Q2" pad="21"/>
<connect gate="A" pin="Q3" pad="20"/>
<connect gate="A" pin="Q4" pad="19"/>
<connect gate="B" pin="CLK" pad="14"/>
<connect gate="B" pin="CLR" pad="13"/>
<connect gate="B" pin="D1" pad="7"/>
<connect gate="B" pin="D2" pad="8"/>
<connect gate="B" pin="D3" pad="9"/>
<connect gate="B" pin="D4" pad="10"/>
<connect gate="B" pin="OC" pad="11"/>
<connect gate="B" pin="Q1" pad="18"/>
<connect gate="B" pin="Q2" pad="17"/>
<connect gate="B" pin="Q3" pad="16"/>
<connect gate="B" pin="Q4" pad="15"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*876" prefix="IC">
<description>2 x 4-bit inverting &lt;b&gt;D type FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74876"/>
<gate name="B" symbol="74876"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="CLK" pad="23"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="OC" pad="2"/>
<connect gate="A" pin="PRE" pad="1"/>
<connect gate="A" pin="Q1" pad="22"/>
<connect gate="A" pin="Q2" pad="21"/>
<connect gate="A" pin="Q3" pad="20"/>
<connect gate="A" pin="Q4" pad="19"/>
<connect gate="B" pin="CLK" pad="14"/>
<connect gate="B" pin="D1" pad="7"/>
<connect gate="B" pin="D2" pad="8"/>
<connect gate="B" pin="D3" pad="9"/>
<connect gate="B" pin="D4" pad="10"/>
<connect gate="B" pin="OC" pad="11"/>
<connect gate="B" pin="PRE" pad="13"/>
<connect gate="B" pin="Q1" pad="18"/>
<connect gate="B" pin="Q2" pad="17"/>
<connect gate="B" pin="Q3" pad="16"/>
<connect gate="B" pin="Q4" pad="15"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*877" prefix="IC">
<description>Universal &lt;b&gt;BUS DRIVER/PORT CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74877"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="A1" pad="4"/>
<connect gate="A" pin="A2" pad="5"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="7"/>
<connect gate="A" pin="A5" pad="8"/>
<connect gate="A" pin="A6" pad="9"/>
<connect gate="A" pin="A7" pad="10"/>
<connect gate="A" pin="A8" pad="11"/>
<connect gate="A" pin="B1" pad="21"/>
<connect gate="A" pin="B2" pad="20"/>
<connect gate="A" pin="B3" pad="19"/>
<connect gate="A" pin="B4" pad="18"/>
<connect gate="A" pin="B5" pad="17"/>
<connect gate="A" pin="B6" pad="16"/>
<connect gate="A" pin="B7" pad="15"/>
<connect gate="A" pin="B8" pad="14"/>
<connect gate="A" pin="CLK" pad="23"/>
<connect gate="A" pin="Q8" pad="13"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="3"/>
<connect gate="A" pin="SRI" pad="22"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*879" prefix="IC">
<description>2 x 4-bit inverting D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74879"/>
<gate name="B" symbol="74879"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="CLK" pad="23"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="OC" pad="2"/>
<connect gate="A" pin="Q1" pad="22"/>
<connect gate="A" pin="Q2" pad="21"/>
<connect gate="A" pin="Q3" pad="20"/>
<connect gate="A" pin="Q4" pad="19"/>
<connect gate="B" pin="CLK" pad="14"/>
<connect gate="B" pin="CLR" pad="13"/>
<connect gate="B" pin="D1" pad="7"/>
<connect gate="B" pin="D2" pad="8"/>
<connect gate="B" pin="D3" pad="9"/>
<connect gate="B" pin="D4" pad="10"/>
<connect gate="B" pin="OC" pad="11"/>
<connect gate="B" pin="Q1" pad="18"/>
<connect gate="B" pin="Q2" pad="17"/>
<connect gate="B" pin="Q3" pad="16"/>
<connect gate="B" pin="Q4" pad="15"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*880" prefix="IC">
<description>2 x 4-bit inverting D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74880"/>
<gate name="B" symbol="74880"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="C" pad="23"/>
<connect gate="A" pin="D1" pad="3"/>
<connect gate="A" pin="D2" pad="4"/>
<connect gate="A" pin="D3" pad="5"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="OC" pad="2"/>
<connect gate="A" pin="PRE" pad="1"/>
<connect gate="A" pin="Q1" pad="22"/>
<connect gate="A" pin="Q2" pad="21"/>
<connect gate="A" pin="Q3" pad="20"/>
<connect gate="A" pin="Q4" pad="19"/>
<connect gate="B" pin="C" pad="14"/>
<connect gate="B" pin="D1" pad="7"/>
<connect gate="B" pin="D2" pad="8"/>
<connect gate="B" pin="D3" pad="9"/>
<connect gate="B" pin="D4" pad="10"/>
<connect gate="B" pin="OC" pad="11"/>
<connect gate="B" pin="PRE" pad="13"/>
<connect gate="B" pin="Q1" pad="18"/>
<connect gate="B" pin="Q2" pad="17"/>
<connect gate="B" pin="Q3" pad="16"/>
<connect gate="B" pin="Q4" pad="15"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*882" prefix="IC">
<description>&lt;b&gt;CARRY GENERATOR&lt;/b&gt; for 32-bit ALU</description>
<gates>
<gate name="A" symbol="74882"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="CN" pad="1"/>
<connect gate="A" pin="CN+16" pad="11"/>
<connect gate="A" pin="CN+24" pad="17"/>
<connect gate="A" pin="CN+32" pad="22"/>
<connect gate="A" pin="CN+8" pad="6"/>
<connect gate="A" pin="G0" pad="2"/>
<connect gate="A" pin="G1" pad="4"/>
<connect gate="A" pin="G2" pad="7"/>
<connect gate="A" pin="G3" pad="9"/>
<connect gate="A" pin="G4" pad="13"/>
<connect gate="A" pin="G5" pad="15"/>
<connect gate="A" pin="G6" pad="18"/>
<connect gate="A" pin="G7" pad="20"/>
<connect gate="A" pin="P0" pad="3"/>
<connect gate="A" pin="P1" pad="5"/>
<connect gate="A" pin="P2" pad="8"/>
<connect gate="A" pin="P3" pad="10"/>
<connect gate="A" pin="P4" pad="14"/>
<connect gate="A" pin="P5" pad="16"/>
<connect gate="A" pin="P6" pad="19"/>
<connect gate="A" pin="P7" pad="21"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*885" prefix="IC">
<description>Expandable 8-bit magnitude &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74885"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="L/!A" pad="1"/>
<connect gate="A" pin="P0" pad="15"/>
<connect gate="A" pin="P1" pad="16"/>
<connect gate="A" pin="P2" pad="17"/>
<connect gate="A" pin="P3" pad="18"/>
<connect gate="A" pin="P4" pad="19"/>
<connect gate="A" pin="P5" pad="20"/>
<connect gate="A" pin="P6" pad="21"/>
<connect gate="A" pin="P7" pad="22"/>
<connect gate="A" pin="P&lt;Q_0" pad="14"/>
<connect gate="A" pin="P&lt;Q_I" pad="2"/>
<connect gate="A" pin="P&gt;Q_I" pad="3"/>
<connect gate="A" pin="P&gt;Q_O" pad="13"/>
<connect gate="A" pin="PLE" pad="23"/>
<connect gate="A" pin="Q0" pad="11"/>
<connect gate="A" pin="Q1" pad="10"/>
<connect gate="A" pin="Q2" pad="9"/>
<connect gate="A" pin="Q3" pad="8"/>
<connect gate="A" pin="Q4" pad="7"/>
<connect gate="A" pin="Q5" pad="6"/>
<connect gate="A" pin="Q6" pad="5"/>
<connect gate="A" pin="Q7" pad="4"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*757" prefix="IC">
<description>8-bit &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74757"/>
<gate name="B" symbol="74757"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*760" prefix="IC">
<description>8-bit &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74757"/>
<gate name="B" symbol="74757"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="8"/>
<connect gate="A" pin="G" pad="1"/>
<connect gate="A" pin="Y1" pad="18"/>
<connect gate="A" pin="Y2" pad="16"/>
<connect gate="A" pin="Y3" pad="14"/>
<connect gate="A" pin="Y4" pad="12"/>
<connect gate="B" pin="A1" pad="11"/>
<connect gate="B" pin="A2" pad="13"/>
<connect gate="B" pin="A3" pad="15"/>
<connect gate="B" pin="A4" pad="17"/>
<connect gate="B" pin="G" pad="19"/>
<connect gate="B" pin="Y1" pad="9"/>
<connect gate="B" pin="Y2" pad="7"/>
<connect gate="B" pin="Y3" pad="5"/>
<connect gate="B" pin="Y4" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*693" prefix="IC">
<description>Synchronous &lt;b&gt;BINARY COUNTER&lt;/b&gt;, register, 3-state</description>
<gates>
<gate name="A" symbol="74690"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CCK" pad="2"/>
<connect gate="A" pin="CCL" pad="1"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="14"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="LD" pad="13"/>
<connect gate="A" pin="QA" pad="18"/>
<connect gate="A" pin="QB" pad="17"/>
<connect gate="A" pin="QC" pad="16"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="R/!C" pad="11"/>
<connect gate="A" pin="RCK" pad="9"/>
<connect gate="A" pin="RCL" pad="8"/>
<connect gate="A" pin="RCO" pad="19"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*699" prefix="IC">
<description>Synchronous binary &lt;b&gt;UP/DOWN COUNTER&lt;/b&gt;, register, 3-state</description>
<gates>
<gate name="A" symbol="74696"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CCK" pad="2"/>
<connect gate="A" pin="CCL" pad="8"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="14"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="LD" pad="13"/>
<connect gate="A" pin="QA" pad="18"/>
<connect gate="A" pin="QB" pad="17"/>
<connect gate="A" pin="QC" pad="16"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="R/!C" pad="11"/>
<connect gate="A" pin="RCK" pad="9"/>
<connect gate="A" pin="RCO" pad="19"/>
<connect gate="A" pin="U/!D" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="DW" package="SO20W">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CCK" pad="2"/>
<connect gate="A" pin="CCL" pad="8"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="14"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="LD" pad="13"/>
<connect gate="A" pin="QA" pad="18"/>
<connect gate="A" pin="QB" pad="17"/>
<connect gate="A" pin="QC" pad="16"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="R/!C" pad="11"/>
<connect gate="A" pin="RCK" pad="9"/>
<connect gate="A" pin="RCO" pad="19"/>
<connect gate="A" pin="U/!D" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="4"/>
<connect gate="A" pin="C" pad="5"/>
<connect gate="A" pin="CCK" pad="2"/>
<connect gate="A" pin="CCL" pad="8"/>
<connect gate="A" pin="D" pad="6"/>
<connect gate="A" pin="ENP" pad="7"/>
<connect gate="A" pin="ENT" pad="14"/>
<connect gate="A" pin="G" pad="12"/>
<connect gate="A" pin="LD" pad="13"/>
<connect gate="A" pin="QA" pad="18"/>
<connect gate="A" pin="QB" pad="17"/>
<connect gate="A" pin="QC" pad="16"/>
<connect gate="A" pin="QD" pad="15"/>
<connect gate="A" pin="R/!C" pad="11"/>
<connect gate="A" pin="RCK" pad="9"/>
<connect gate="A" pin="RCO" pad="19"/>
<connect gate="A" pin="U/!D" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*533" prefix="IC">
<description>Inverting 8-bit D type &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74533"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*534" prefix="IC">
<description>8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74534"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="5"/>
<connect gate="A" pin="3D" pad="7"/>
<connect gate="A" pin="3Q" pad="6"/>
<connect gate="A" pin="4D" pad="8"/>
<connect gate="A" pin="4Q" pad="9"/>
<connect gate="A" pin="5D" pad="13"/>
<connect gate="A" pin="5Q" pad="12"/>
<connect gate="A" pin="6D" pad="14"/>
<connect gate="A" pin="6Q" pad="15"/>
<connect gate="A" pin="7D" pad="17"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="19"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*563" prefix="IC">
<description>Inverting 8-bit D type &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74563"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="19"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="18"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="17"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="16"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="15"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="14"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="13"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="HC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*564" prefix="IC">
<description>Inverting 8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74564"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="19"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="18"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="17"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="16"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="15"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="14"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="13"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="HC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*573" prefix="IC">
<description>8-bit D latch &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74573"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="19"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="18"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="17"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="16"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="15"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="14"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="13"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
<technology name="HC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*574" prefix="IC">
<description>8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt; bus driver</description>
<gates>
<gate name="A" symbol="74574"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="19"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="18"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="17"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="16"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="15"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="14"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="13"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
<technology name="HC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*575" prefix="IC">
<description>8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74575"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="22"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="21"/>
<connect gate="A" pin="3D" pad="5"/>
<connect gate="A" pin="3Q" pad="20"/>
<connect gate="A" pin="4D" pad="6"/>
<connect gate="A" pin="4Q" pad="19"/>
<connect gate="A" pin="5D" pad="7"/>
<connect gate="A" pin="5Q" pad="18"/>
<connect gate="A" pin="6D" pad="8"/>
<connect gate="A" pin="6Q" pad="17"/>
<connect gate="A" pin="7D" pad="9"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="10"/>
<connect gate="A" pin="8Q" pad="15"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="OC" pad="2"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*576" prefix="IC">
<description>Inverting 8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74576"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="19"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="18"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="17"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="16"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="15"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="14"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="13"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*577" prefix="IC">
<description>Inverting 8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74577"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="22"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="21"/>
<connect gate="A" pin="3D" pad="5"/>
<connect gate="A" pin="3Q" pad="20"/>
<connect gate="A" pin="4D" pad="6"/>
<connect gate="A" pin="4Q" pad="19"/>
<connect gate="A" pin="5D" pad="7"/>
<connect gate="A" pin="5Q" pad="18"/>
<connect gate="A" pin="6D" pad="8"/>
<connect gate="A" pin="6Q" pad="17"/>
<connect gate="A" pin="7D" pad="9"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="10"/>
<connect gate="A" pin="8Q" pad="15"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="OC" pad="2"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*580" prefix="IC">
<description>Inverting 8-bit D type &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74580"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="19"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="18"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="17"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="16"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="15"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="14"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="13"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="C" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*821" prefix="IC">
<description>10-bit bus interface &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74821"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="10D" pad="11"/>
<connect gate="A" pin="10Q" pad="14"/>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="23"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="22"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="21"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="20"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="19"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="18"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="17"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="16"/>
<connect gate="A" pin="9D" pad="10"/>
<connect gate="A" pin="9Q" pad="15"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*822" prefix="IC">
<description>10-bit inverting bus interface &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74822"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="10D" pad="11"/>
<connect gate="A" pin="10Q" pad="14"/>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="23"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="22"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="21"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="20"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="19"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="18"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="17"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="16"/>
<connect gate="A" pin="9D" pad="10"/>
<connect gate="A" pin="9Q" pad="15"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*823" prefix="IC">
<description>9-bit bus interface &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74823"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="23"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="22"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="21"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="20"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="19"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="18"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="17"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="16"/>
<connect gate="A" pin="9D" pad="10"/>
<connect gate="A" pin="9Q" pad="15"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="CLKEN" pad="14"/>
<connect gate="A" pin="CLR" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*824" prefix="IC">
<description>9-bit inverting bus interface &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74824"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="1D" pad="2"/>
<connect gate="A" pin="1Q" pad="23"/>
<connect gate="A" pin="2D" pad="3"/>
<connect gate="A" pin="2Q" pad="22"/>
<connect gate="A" pin="3D" pad="4"/>
<connect gate="A" pin="3Q" pad="21"/>
<connect gate="A" pin="4D" pad="5"/>
<connect gate="A" pin="4Q" pad="20"/>
<connect gate="A" pin="5D" pad="6"/>
<connect gate="A" pin="5Q" pad="19"/>
<connect gate="A" pin="6D" pad="7"/>
<connect gate="A" pin="6Q" pad="18"/>
<connect gate="A" pin="7D" pad="8"/>
<connect gate="A" pin="7Q" pad="17"/>
<connect gate="A" pin="8D" pad="9"/>
<connect gate="A" pin="8Q" pad="16"/>
<connect gate="A" pin="9D" pad="10"/>
<connect gate="A" pin="9Q" pad="15"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="CLKEN" pad="14"/>
<connect gate="A" pin="CLR" pad="11"/>
<connect gate="A" pin="OC" pad="1"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*825" prefix="IC">
<description>8-bit bus interface &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74825"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="22"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="21"/>
<connect gate="A" pin="3D" pad="5"/>
<connect gate="A" pin="3Q" pad="20"/>
<connect gate="A" pin="4D" pad="6"/>
<connect gate="A" pin="4Q" pad="19"/>
<connect gate="A" pin="5D" pad="7"/>
<connect gate="A" pin="5Q" pad="18"/>
<connect gate="A" pin="6D" pad="8"/>
<connect gate="A" pin="6Q" pad="17"/>
<connect gate="A" pin="7D" pad="9"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="10"/>
<connect gate="A" pin="8Q" pad="15"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="CLKEN" pad="14"/>
<connect gate="A" pin="CLR" pad="11"/>
<connect gate="A" pin="OC1" pad="1"/>
<connect gate="A" pin="OC2" pad="2"/>
<connect gate="A" pin="OC3" pad="23"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*826" prefix="IC">
<description>8-bit inverting bus interface &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74826"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-6">
<connects>
<connect gate="A" pin="1D" pad="3"/>
<connect gate="A" pin="1Q" pad="22"/>
<connect gate="A" pin="2D" pad="4"/>
<connect gate="A" pin="2Q" pad="21"/>
<connect gate="A" pin="3D" pad="5"/>
<connect gate="A" pin="3Q" pad="20"/>
<connect gate="A" pin="4D" pad="6"/>
<connect gate="A" pin="4Q" pad="19"/>
<connect gate="A" pin="5D" pad="7"/>
<connect gate="A" pin="5Q" pad="18"/>
<connect gate="A" pin="6D" pad="8"/>
<connect gate="A" pin="6Q" pad="17"/>
<connect gate="A" pin="7D" pad="9"/>
<connect gate="A" pin="7Q" pad="16"/>
<connect gate="A" pin="8D" pad="10"/>
<connect gate="A" pin="8Q" pad="15"/>
<connect gate="A" pin="CLK" pad="13"/>
<connect gate="A" pin="CLKEN" pad="14"/>
<connect gate="A" pin="CLR" pad="11"/>
<connect gate="A" pin="OC1" pad="1"/>
<connect gate="A" pin="OC2" pad="2"/>
<connect gate="A" pin="OC3" pad="23"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*841" prefix="IC">
<description>10-bit bus interface &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74841"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="NT" package="DIL28-6">
<connects>
<connect gate="A" pin="10D" pad="16"/>
<connect gate="A" pin="10Q" pad="14"/>
<connect gate="A" pin="1D" pad="27"/>
<connect gate="A" pin="1Q" pad="1"/>
<connect gate="A" pin="2D" pad="26"/>
<connect gate="A" pin="2Q" pad="2"/>
<connect gate="A" pin="3D" pad="25"/>
<connect gate="A" pin="3Q" pad="3"/>
<connect gate="A" pin="4D" pad="24"/>
<connect gate="A" pin="4Q" pad="4"/>
<connect gate="A" pin="5D" pad="23"/>
<connect gate="A" pin="5Q" pad="5"/>
<connect gate="A" pin="6D" pad="20"/>
<connect gate="A" pin="6Q" pad="10"/>
<connect gate="A" pin="7D" pad="19"/>
<connect gate="A" pin="7Q" pad="11"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="9D" pad="17"/>
<connect gate="A" pin="9Q" pad="13"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*842" prefix="IC">
<description>10-bit inverting bus interface &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74842"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="NT" package="DIL28-6">
<connects>
<connect gate="A" pin="10D" pad="16"/>
<connect gate="A" pin="10Q" pad="14"/>
<connect gate="A" pin="1D" pad="27"/>
<connect gate="A" pin="1Q" pad="1"/>
<connect gate="A" pin="2D" pad="26"/>
<connect gate="A" pin="2Q" pad="2"/>
<connect gate="A" pin="3D" pad="25"/>
<connect gate="A" pin="3Q" pad="3"/>
<connect gate="A" pin="4D" pad="24"/>
<connect gate="A" pin="4Q" pad="4"/>
<connect gate="A" pin="5D" pad="23"/>
<connect gate="A" pin="5Q" pad="5"/>
<connect gate="A" pin="6D" pad="20"/>
<connect gate="A" pin="6Q" pad="10"/>
<connect gate="A" pin="7D" pad="19"/>
<connect gate="A" pin="7Q" pad="11"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="9D" pad="17"/>
<connect gate="A" pin="9Q" pad="13"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*843" prefix="IC">
<description>9-bit bus interface &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74843"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="NT" package="DIL28-6">
<connects>
<connect gate="A" pin="1D" pad="27"/>
<connect gate="A" pin="1Q" pad="1"/>
<connect gate="A" pin="2D" pad="26"/>
<connect gate="A" pin="2Q" pad="2"/>
<connect gate="A" pin="3D" pad="25"/>
<connect gate="A" pin="3Q" pad="3"/>
<connect gate="A" pin="4D" pad="24"/>
<connect gate="A" pin="4Q" pad="4"/>
<connect gate="A" pin="5D" pad="23"/>
<connect gate="A" pin="5Q" pad="5"/>
<connect gate="A" pin="6D" pad="20"/>
<connect gate="A" pin="6Q" pad="10"/>
<connect gate="A" pin="7D" pad="19"/>
<connect gate="A" pin="7Q" pad="11"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="9D" pad="17"/>
<connect gate="A" pin="9Q" pad="13"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="A" pin="PRE" pad="16"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*844" prefix="IC">
<description>9-bit inverting bus interface &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74844"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="NT" package="DIL28-6">
<connects>
<connect gate="A" pin="1D" pad="27"/>
<connect gate="A" pin="1Q" pad="1"/>
<connect gate="A" pin="2D" pad="26"/>
<connect gate="A" pin="2Q" pad="2"/>
<connect gate="A" pin="3D" pad="25"/>
<connect gate="A" pin="3Q" pad="3"/>
<connect gate="A" pin="4D" pad="24"/>
<connect gate="A" pin="4Q" pad="4"/>
<connect gate="A" pin="5D" pad="23"/>
<connect gate="A" pin="5Q" pad="5"/>
<connect gate="A" pin="6D" pad="20"/>
<connect gate="A" pin="6Q" pad="10"/>
<connect gate="A" pin="7D" pad="19"/>
<connect gate="A" pin="7Q" pad="11"/>
<connect gate="A" pin="8D" pad="18"/>
<connect gate="A" pin="8Q" pad="12"/>
<connect gate="A" pin="9D" pad="17"/>
<connect gate="A" pin="9Q" pad="13"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="OC" pad="28"/>
<connect gate="A" pin="PRE" pad="16"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*845" prefix="IC">
<description>8-bit bus interface &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74845"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="NT" package="DIL28-6">
<connects>
<connect gate="A" pin="1D" pad="26"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="25"/>
<connect gate="A" pin="2Q" pad="3"/>
<connect gate="A" pin="3D" pad="24"/>
<connect gate="A" pin="3Q" pad="4"/>
<connect gate="A" pin="4D" pad="23"/>
<connect gate="A" pin="4Q" pad="5"/>
<connect gate="A" pin="5D" pad="20"/>
<connect gate="A" pin="5Q" pad="10"/>
<connect gate="A" pin="6D" pad="19"/>
<connect gate="A" pin="6Q" pad="11"/>
<connect gate="A" pin="7D" pad="18"/>
<connect gate="A" pin="7Q" pad="12"/>
<connect gate="A" pin="8D" pad="17"/>
<connect gate="A" pin="8Q" pad="13"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="OC1" pad="1"/>
<connect gate="A" pin="OC2" pad="28"/>
<connect gate="A" pin="OC3" pad="27"/>
<connect gate="A" pin="PRE" pad="16"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*846" prefix="IC">
<description>8-bit inverting bus interface &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74846"/>
<gate name="P" symbol="2PWR4GND"/>
</gates>
<devices>
<device name="NT" package="DIL28-6">
<connects>
<connect gate="A" pin="1D" pad="26"/>
<connect gate="A" pin="1Q" pad="2"/>
<connect gate="A" pin="2D" pad="25"/>
<connect gate="A" pin="2Q" pad="3"/>
<connect gate="A" pin="3D" pad="24"/>
<connect gate="A" pin="3Q" pad="4"/>
<connect gate="A" pin="4D" pad="23"/>
<connect gate="A" pin="4Q" pad="5"/>
<connect gate="A" pin="5D" pad="20"/>
<connect gate="A" pin="5Q" pad="10"/>
<connect gate="A" pin="6D" pad="19"/>
<connect gate="A" pin="6Q" pad="11"/>
<connect gate="A" pin="7D" pad="18"/>
<connect gate="A" pin="7Q" pad="12"/>
<connect gate="A" pin="8D" pad="17"/>
<connect gate="A" pin="8Q" pad="13"/>
<connect gate="A" pin="C" pad="15"/>
<connect gate="A" pin="CLR" pad="14"/>
<connect gate="A" pin="OC1" pad="1"/>
<connect gate="A" pin="OC2" pad="28"/>
<connect gate="A" pin="OC3" pad="27"/>
<connect gate="A" pin="PRE" pad="16"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="GND@2" pad="7"/>
<connect gate="P" pin="GND@3" pad="8"/>
<connect gate="P" pin="GND@4" pad="9"/>
<connect gate="P" pin="VCC@1" pad="21"/>
<connect gate="P" pin="VCC@2" pad="22"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*624" prefix="IC">
<description>&lt;b&gt;VOLTAGE CONTROLLED OSCILLATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74624"/>
<gate name="P" symbol="PWRN"/>
<gate name="PO" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="8"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="FCTR" pad="13"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="A" pin="RANGE" pad="2"/>
<connect gate="A" pin="XTC@1" pad="3"/>
<connect gate="A" pin="XTC@2" pad="4"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="9"/>
<connect gate="PO" pin="GND" pad="1"/>
<connect gate="PO" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="!Q" pad="8"/>
<connect gate="A" pin="EN" pad="5"/>
<connect gate="A" pin="FCTR" pad="13"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="A" pin="RANGE" pad="2"/>
<connect gate="A" pin="XTC@1" pad="3"/>
<connect gate="A" pin="XTC@2" pad="4"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="9"/>
<connect gate="PO" pin="GND" pad="1"/>
<connect gate="PO" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*20" prefix="IC">
<description>Dual 4-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7420"/>
<gate name="B" symbol="7420"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="B" pin="I0" pad="9"/>
<connect gate="B" pin="I1" pad="10"/>
<connect gate="B" pin="I2" pad="12"/>
<connect gate="B" pin="I3" pad="13"/>
<connect gate="B" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="I2" pad="4"/>
<connect gate="A" pin="I3" pad="5"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="B" pin="I0" pad="9"/>
<connect gate="B" pin="I1" pad="10"/>
<connect gate="B" pin="I2" pad="12"/>
<connect gate="B" pin="I3" pad="13"/>
<connect gate="B" pin="O" pad="8"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="I2" pad="6"/>
<connect gate="A" pin="I3" pad="8"/>
<connect gate="A" pin="O" pad="9"/>
<connect gate="B" pin="I0" pad="13"/>
<connect gate="B" pin="I1" pad="14"/>
<connect gate="B" pin="I2" pad="18"/>
<connect gate="B" pin="I3" pad="19"/>
<connect gate="B" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="ALS"/>
<technology name="AS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*36" prefix="IC">
<description>Quad 2-input &lt;b&gt;NOR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7436"/>
<gate name="B" symbol="7436"/>
<gate name="C" symbol="7436"/>
<gate name="D" symbol="7436"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*37" prefix="IC">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; buffer</description>
<gates>
<gate name="A" symbol="7437"/>
<gate name="B" symbol="7437"/>
<gate name="C" symbol="7437"/>
<gate name="D" symbol="7437"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="3"/>
<connect gate="B" pin="I0" pad="4"/>
<connect gate="B" pin="I1" pad="5"/>
<connect gate="B" pin="O" pad="6"/>
<connect gate="C" pin="I0" pad="9"/>
<connect gate="C" pin="I1" pad="10"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I0" pad="12"/>
<connect gate="D" pin="I1" pad="13"/>
<connect gate="D" pin="O" pad="11"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
<device name="FK" package="LCC20">
<connects>
<connect gate="A" pin="I0" pad="2"/>
<connect gate="A" pin="I1" pad="3"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="B" pin="I0" pad="6"/>
<connect gate="B" pin="I1" pad="8"/>
<connect gate="B" pin="O" pad="9"/>
<connect gate="C" pin="I0" pad="13"/>
<connect gate="C" pin="I1" pad="14"/>
<connect gate="C" pin="O" pad="12"/>
<connect gate="D" pin="I0" pad="18"/>
<connect gate="D" pin="I1" pad="19"/>
<connect gate="D" pin="O" pad="16"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
<technology name="ALS"/>
<technology name="LS"/>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*303" prefix="IC">
<description>Octal devide by 2 &lt;b&gt;CIRCUITS/CLOCK DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="74303"/>
<gate name="P" symbol="2PWR3GND"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="CLK" pad="11"/>
<connect gate="G$1" pin="CLR" pad="14"/>
<connect gate="G$1" pin="PRE" pad="10"/>
<connect gate="G$1" pin="Q1" pad="15"/>
<connect gate="G$1" pin="Q2" pad="16"/>
<connect gate="G$1" pin="Q3" pad="1"/>
<connect gate="G$1" pin="Q4" pad="2"/>
<connect gate="G$1" pin="Q5" pad="6"/>
<connect gate="G$1" pin="Q6" pad="7"/>
<connect gate="G$1" pin="Q7" pad="8"/>
<connect gate="G$1" pin="Q8" pad="9"/>
<connect gate="P" pin="GND@1" pad="3"/>
<connect gate="P" pin="GND@2" pad="4"/>
<connect gate="P" pin="GND@3" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*304" prefix="IC">
<description>Octal devide by 2 &lt;b&gt;CIRCUITS/CLOCK DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="74304"/>
<gate name="P" symbol="2PWR3GND"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="CLK" pad="11"/>
<connect gate="G$1" pin="CLR" pad="14"/>
<connect gate="G$1" pin="PRE" pad="10"/>
<connect gate="G$1" pin="Q1" pad="15"/>
<connect gate="G$1" pin="Q2" pad="16"/>
<connect gate="G$1" pin="Q3" pad="1"/>
<connect gate="G$1" pin="Q4" pad="2"/>
<connect gate="G$1" pin="Q5" pad="6"/>
<connect gate="G$1" pin="Q6" pad="7"/>
<connect gate="G$1" pin="Q7" pad="8"/>
<connect gate="G$1" pin="Q8" pad="9"/>
<connect gate="P" pin="GND@1" pad="3"/>
<connect gate="P" pin="GND@2" pad="4"/>
<connect gate="P" pin="GND@3" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*305" prefix="IC">
<description>Octal devide by 2 &lt;b&gt;CIRCUITS/CLOCK DRIVER&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="2PWR3GND"/>
<gate name="A" symbol="74305"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CLK" pad="11"/>
<connect gate="A" pin="PRE" pad="10"/>
<connect gate="A" pin="Q1" pad="15"/>
<connect gate="A" pin="Q2" pad="16"/>
<connect gate="A" pin="Q3" pad="1"/>
<connect gate="A" pin="Q4" pad="2"/>
<connect gate="A" pin="Q5" pad="6"/>
<connect gate="A" pin="Q6" pad="7"/>
<connect gate="A" pin="Q7" pad="8"/>
<connect gate="A" pin="Q8" pad="9"/>
<connect gate="A" pin="RST" pad="14"/>
<connect gate="P" pin="GND@1" pad="3"/>
<connect gate="P" pin="GND@2" pad="4"/>
<connect gate="P" pin="GND@3" pad="5"/>
<connect gate="P" pin="VCC@1" pad="12"/>
<connect gate="P" pin="VCC@2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*60" prefix="IC">
<description>Dual 4-input &lt;b&gt;EXPANDER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7460"/>
<gate name="B" symbol="7460"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!X" pad="12"/>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="3"/>
<connect gate="A" pin="D" pad="13"/>
<connect gate="A" pin="X" pad="11"/>
<connect gate="B" pin="!X" pad="9"/>
<connect gate="B" pin="A" pad="4"/>
<connect gate="B" pin="B" pad="5"/>
<connect gate="B" pin="C" pad="6"/>
<connect gate="B" pin="D" pad="8"/>
<connect gate="B" pin="X" pad="10"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*80" prefix="IC">
<description>1-bit full &lt;b&gt;ADDER&lt;/b&gt;,, parallel carry</description>
<gates>
<gate name="A" symbol="7480"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!S" pad="6"/>
<connect gate="A" pin="A*" pad="10"/>
<connect gate="A" pin="A1" pad="8"/>
<connect gate="A" pin="A2" pad="9"/>
<connect gate="A" pin="AC" pad="11"/>
<connect gate="A" pin="B*" pad="1"/>
<connect gate="A" pin="B1" pad="12"/>
<connect gate="A" pin="B2" pad="13"/>
<connect gate="A" pin="BC" pad="2"/>
<connect gate="A" pin="CN" pad="3"/>
<connect gate="A" pin="CN+1" pad="4"/>
<connect gate="A" pin="S" pad="5"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*94" prefix="IC">
<description>4-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, parallel NOR inputs, serial output</description>
<gates>
<gate name="A" symbol="7494"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="CLK" pad="8"/>
<connect gate="A" pin="CLR" pad="10"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="P1A" pad="1"/>
<connect gate="A" pin="P1B" pad="2"/>
<connect gate="A" pin="P1C" pad="3"/>
<connect gate="A" pin="P1D" pad="4"/>
<connect gate="A" pin="P2A" pad="16"/>
<connect gate="A" pin="P2B" pad="14"/>
<connect gate="A" pin="P2C" pad="13"/>
<connect gate="A" pin="P2D" pad="11"/>
<connect gate="A" pin="PE1" pad="6"/>
<connect gate="A" pin="PE2" pad="15"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="SO16">
<connects>
<connect gate="A" pin="CLK" pad="8"/>
<connect gate="A" pin="CLR" pad="10"/>
<connect gate="A" pin="IN" pad="7"/>
<connect gate="A" pin="OUT" pad="9"/>
<connect gate="A" pin="P1A" pad="1"/>
<connect gate="A" pin="P1B" pad="2"/>
<connect gate="A" pin="P1C" pad="3"/>
<connect gate="A" pin="P1D" pad="4"/>
<connect gate="A" pin="P2A" pad="16"/>
<connect gate="A" pin="P2B" pad="14"/>
<connect gate="A" pin="P2C" pad="13"/>
<connect gate="A" pin="P2D" pad="11"/>
<connect gate="A" pin="PE1" pad="6"/>
<connect gate="A" pin="PE2" pad="15"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*105" prefix="IC">
<description>Single J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74105"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="8"/>
<connect gate="A" pin="CLK" pad="9"/>
<connect gate="A" pin="CLR" pad="13"/>
<connect gate="A" pin="J1" pad="4"/>
<connect gate="A" pin="J2" pad="5"/>
<connect gate="A" pin="J3" pad="12"/>
<connect gate="A" pin="JK" pad="1"/>
<connect gate="A" pin="K1" pad="3"/>
<connect gate="A" pin="K2" pad="10"/>
<connect gate="A" pin="K3" pad="11"/>
<connect gate="A" pin="PRE" pad="2"/>
<connect gate="A" pin="Q" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*141" prefix="IC">
<description>BCD to decimal &lt;b&gt;DECODER/DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74141"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="0" pad="16"/>
<connect gate="A" pin="1" pad="15"/>
<connect gate="A" pin="2" pad="8"/>
<connect gate="A" pin="3" pad="9"/>
<connect gate="A" pin="4" pad="13"/>
<connect gate="A" pin="5" pad="14"/>
<connect gate="A" pin="6" pad="11"/>
<connect gate="A" pin="7" pad="10"/>
<connect gate="A" pin="8" pad="1"/>
<connect gate="A" pin="9" pad="2"/>
<connect gate="A" pin="A" pad="3"/>
<connect gate="A" pin="B" pad="6"/>
<connect gate="A" pin="C" pad="7"/>
<connect gate="A" pin="D" pad="4"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*142" prefix="IC">
<description>Decimal &lt;b&gt;COUNTER&lt;/b&gt; and BCD to decimal &lt;b&gt;DECODER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74142"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="0" pad="10"/>
<connect gate="A" pin="1" pad="9"/>
<connect gate="A" pin="2" pad="7"/>
<connect gate="A" pin="3" pad="6"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="3"/>
<connect gate="A" pin="7" pad="2"/>
<connect gate="A" pin="8" pad="11"/>
<connect gate="A" pin="9" pad="12"/>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="QD" pad="14"/>
<connect gate="A" pin="STRB" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="J" package="SO16">
<connects>
<connect gate="A" pin="0" pad="10"/>
<connect gate="A" pin="1" pad="9"/>
<connect gate="A" pin="2" pad="7"/>
<connect gate="A" pin="3" pad="6"/>
<connect gate="A" pin="4" pad="4"/>
<connect gate="A" pin="5" pad="5"/>
<connect gate="A" pin="6" pad="3"/>
<connect gate="A" pin="7" pad="2"/>
<connect gate="A" pin="8" pad="11"/>
<connect gate="A" pin="9" pad="12"/>
<connect gate="A" pin="CLK" pad="15"/>
<connect gate="A" pin="CLR" pad="1"/>
<connect gate="A" pin="QD" pad="14"/>
<connect gate="A" pin="STRB" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*172" prefix="IC">
<description>16-bit multiple port &lt;b&gt;REGISTER&lt;/b&gt;, 3-state ouput</description>
<gates>
<gate name="A" symbol="74172"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="A" pin="1DA" pad="22"/>
<connect gate="A" pin="1DB" pad="4"/>
<connect gate="A" pin="1GR" pad="15"/>
<connect gate="A" pin="1GW" pad="3"/>
<connect gate="A" pin="1QA" pad="14"/>
<connect gate="A" pin="1QB" pad="10"/>
<connect gate="A" pin="1R0" pad="9"/>
<connect gate="A" pin="1R1" pad="8"/>
<connect gate="A" pin="1R2" pad="7"/>
<connect gate="A" pin="1W0" pad="2"/>
<connect gate="A" pin="1W1" pad="1"/>
<connect gate="A" pin="1W2" pad="23"/>
<connect gate="A" pin="2DA" pad="21"/>
<connect gate="A" pin="2DB" pad="5"/>
<connect gate="A" pin="2GR" pad="16"/>
<connect gate="A" pin="2GW" pad="20"/>
<connect gate="A" pin="2QA" pad="13"/>
<connect gate="A" pin="2QB" pad="11"/>
<connect gate="A" pin="2W/R0" pad="17"/>
<connect gate="A" pin="2W/R1" pad="18"/>
<connect gate="A" pin="2W/R2" pad="19"/>
<connect gate="A" pin="CLK" pad="6"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*226" prefix="IC">
<description>4-bit bidirectional &lt;b&gt;BUS DRIVER&lt;/b&gt;, buffer</description>
<gates>
<gate name="A" symbol="74226"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="B1" pad="13"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="11"/>
<connect gate="A" pin="B4" pad="10"/>
<connect gate="A" pin="GAB" pad="15"/>
<connect gate="A" pin="GBA" pad="1"/>
<connect gate="A" pin="OCAB" pad="9"/>
<connect gate="A" pin="OCBA" pad="7"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="J" package="SO16">
<connects>
<connect gate="A" pin="A1" pad="3"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="5"/>
<connect gate="A" pin="A4" pad="6"/>
<connect gate="A" pin="B1" pad="13"/>
<connect gate="A" pin="B2" pad="12"/>
<connect gate="A" pin="B3" pad="11"/>
<connect gate="A" pin="B4" pad="10"/>
<connect gate="A" pin="GAB" pad="15"/>
<connect gate="A" pin="GBA" pad="1"/>
<connect gate="A" pin="OCAB" pad="9"/>
<connect gate="A" pin="OCBA" pad="7"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="14"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*274" prefix="IC">
<description>4 by 4-bit &lt;b&gt;MULTIPLIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74274"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="AN" pad="1"/>
<connect gate="A" pin="AN1" pad="2"/>
<connect gate="A" pin="AN2" pad="3"/>
<connect gate="A" pin="AN3" pad="4"/>
<connect gate="A" pin="BN" pad="5"/>
<connect gate="A" pin="BN1" pad="17"/>
<connect gate="A" pin="BN2" pad="18"/>
<connect gate="A" pin="BN3" pad="19"/>
<connect gate="A" pin="G1" pad="15"/>
<connect gate="A" pin="G2" pad="16"/>
<connect gate="A" pin="N" pad="6"/>
<connect gate="A" pin="N+1" pad="7"/>
<connect gate="A" pin="N+2" pad="8"/>
<connect gate="A" pin="N+3" pad="9"/>
<connect gate="A" pin="N+4" pad="11"/>
<connect gate="A" pin="N+5" pad="12"/>
<connect gate="A" pin="N+6" pad="13"/>
<connect gate="A" pin="N+7" pad="14"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="J" package="SO20W">
<connects>
<connect gate="A" pin="AN" pad="1"/>
<connect gate="A" pin="AN1" pad="2"/>
<connect gate="A" pin="AN2" pad="3"/>
<connect gate="A" pin="AN3" pad="4"/>
<connect gate="A" pin="BN" pad="5"/>
<connect gate="A" pin="BN1" pad="17"/>
<connect gate="A" pin="BN2" pad="18"/>
<connect gate="A" pin="BN3" pad="19"/>
<connect gate="A" pin="G1" pad="15"/>
<connect gate="A" pin="G2" pad="16"/>
<connect gate="A" pin="N" pad="6"/>
<connect gate="A" pin="N+1" pad="7"/>
<connect gate="A" pin="N+2" pad="8"/>
<connect gate="A" pin="N+3" pad="9"/>
<connect gate="A" pin="N+4" pad="11"/>
<connect gate="A" pin="N+5" pad="12"/>
<connect gate="A" pin="N+6" pad="13"/>
<connect gate="A" pin="N+7" pad="14"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*275" prefix="IC">
<description>7-bit &lt;b&gt;WALLACE TREE&lt;/b&gt; element</description>
<gates>
<gate name="A" symbol="74275"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="2N+0" pad="9"/>
<connect gate="A" pin="2N+1" pad="11"/>
<connect gate="A" pin="2N+2" pad="12"/>
<connect gate="A" pin="2N@1" pad="1"/>
<connect gate="A" pin="2N@2" pad="2"/>
<connect gate="A" pin="2N@3" pad="3"/>
<connect gate="A" pin="2N@4" pad="4"/>
<connect gate="A" pin="2N@5" pad="7"/>
<connect gate="A" pin="2N@6" pad="14"/>
<connect gate="A" pin="2N@7" pad="15"/>
<connect gate="A" pin="C2N+1" pad="10"/>
<connect gate="A" pin="C2N@1" pad="5"/>
<connect gate="A" pin="C2N@2" pad="6"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="J" package="SO16">
<connects>
<connect gate="A" pin="2N+0" pad="9"/>
<connect gate="A" pin="2N+1" pad="11"/>
<connect gate="A" pin="2N+2" pad="12"/>
<connect gate="A" pin="2N@1" pad="1"/>
<connect gate="A" pin="2N@2" pad="2"/>
<connect gate="A" pin="2N@3" pad="3"/>
<connect gate="A" pin="2N@4" pad="4"/>
<connect gate="A" pin="2N@5" pad="7"/>
<connect gate="A" pin="2N@6" pad="14"/>
<connect gate="A" pin="2N@7" pad="15"/>
<connect gate="A" pin="C2N+1" pad="10"/>
<connect gate="A" pin="C2N@1" pad="5"/>
<connect gate="A" pin="C2N@2" pad="6"/>
<connect gate="A" pin="G" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*428" prefix="IC">
<description>&lt;b&gt;SYSTEM CONTROLLER/BUS DRIVER&lt;/b&gt; for 8080 (=Intel 8228)</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="A" symbol="74428"/>
</gates>
<devices>
<device name="N" package="DIL28-6">
<connects>
<connect gate="A" pin="BUSEN" pad="22"/>
<connect gate="A" pin="D0" pad="15"/>
<connect gate="A" pin="D1" pad="17"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="D3" pad="10"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="21"/>
<connect gate="A" pin="D7" pad="8"/>
<connect gate="A" pin="DB0" pad="13"/>
<connect gate="A" pin="DB1" pad="16"/>
<connect gate="A" pin="DB2" pad="11"/>
<connect gate="A" pin="DB3" pad="9"/>
<connect gate="A" pin="DB4" pad="5"/>
<connect gate="A" pin="DB5" pad="18"/>
<connect gate="A" pin="DB6" pad="20"/>
<connect gate="A" pin="DB7" pad="7"/>
<connect gate="A" pin="DBIN" pad="4"/>
<connect gate="A" pin="HLDA" pad="2"/>
<connect gate="A" pin="I/OR" pad="25"/>
<connect gate="A" pin="I/OW" pad="27"/>
<connect gate="A" pin="INTA" pad="23"/>
<connect gate="A" pin="MEMR" pad="24"/>
<connect gate="A" pin="MEMW" pad="26"/>
<connect gate="A" pin="STSTB" pad="1"/>
<connect gate="A" pin="WR" pad="3"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*436" prefix="IC">
<description>Hex inverting &lt;b&gt;LINE DRIVER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74436"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="10"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="15"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
<device name="J" package="SO16">
<connects>
<connect gate="A" pin="A1" pad="2"/>
<connect gate="A" pin="A2" pad="4"/>
<connect gate="A" pin="A3" pad="6"/>
<connect gate="A" pin="A4" pad="10"/>
<connect gate="A" pin="A5" pad="12"/>
<connect gate="A" pin="A6" pad="14"/>
<connect gate="A" pin="G1" pad="1"/>
<connect gate="A" pin="G2" pad="15"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="5"/>
<connect gate="A" pin="Y3" pad="7"/>
<connect gate="A" pin="Y4" pad="9"/>
<connect gate="A" pin="Y5" pad="11"/>
<connect gate="A" pin="Y6" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*543" prefix="IC">
<description>8-bit bidirectional &lt;b&gt;BUS DRIVER&lt;/b&gt;, latch</description>
<gates>
<gate name="G$1" symbol="74543"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="10"/>
<connect gate="G$1" pin="B1" pad="22"/>
<connect gate="G$1" pin="B2" pad="21"/>
<connect gate="G$1" pin="B3" pad="20"/>
<connect gate="G$1" pin="B4" pad="19"/>
<connect gate="G$1" pin="B5" pad="18"/>
<connect gate="G$1" pin="B6" pad="17"/>
<connect gate="G$1" pin="B7" pad="16"/>
<connect gate="G$1" pin="B8" pad="15"/>
<connect gate="G$1" pin="CEAB" pad="11"/>
<connect gate="G$1" pin="CEBA" pad="23"/>
<connect gate="G$1" pin="GAB" pad="13"/>
<connect gate="G$1" pin="GBA" pad="2"/>
<connect gate="G$1" pin="LEAB" pad="14"/>
<connect gate="G$1" pin="LEBA" pad="1"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="HCT"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*634" prefix="IC">
<description>32-bit &lt;b&gt;EDAC&lt;/b&gt; error detection and correction</description>
<gates>
<gate name="A" symbol="74634"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="JD" package="DIL48">
<connects>
<connect gate="A" pin="CB0" pad="28"/>
<connect gate="A" pin="CB1" pad="27"/>
<connect gate="A" pin="CB2" pad="26"/>
<connect gate="A" pin="CB3" pad="25"/>
<connect gate="A" pin="CB4" pad="23"/>
<connect gate="A" pin="CB5" pad="22"/>
<connect gate="A" pin="CB6" pad="21"/>
<connect gate="A" pin="DB0" pad="3"/>
<connect gate="A" pin="DB1" pad="4"/>
<connect gate="A" pin="DB10" pad="15"/>
<connect gate="A" pin="DB11" pad="16"/>
<connect gate="A" pin="DB12" pad="17"/>
<connect gate="A" pin="DB13" pad="18"/>
<connect gate="A" pin="DB14" pad="19"/>
<connect gate="A" pin="DB15" pad="20"/>
<connect gate="A" pin="DB16" pad="29"/>
<connect gate="A" pin="DB17" pad="30"/>
<connect gate="A" pin="DB18" pad="31"/>
<connect gate="A" pin="DB19" pad="32"/>
<connect gate="A" pin="DB2" pad="5"/>
<connect gate="A" pin="DB20" pad="33"/>
<connect gate="A" pin="DB21" pad="34"/>
<connect gate="A" pin="DB22" pad="35"/>
<connect gate="A" pin="DB23" pad="36"/>
<connect gate="A" pin="DB24" pad="38"/>
<connect gate="A" pin="DB25" pad="39"/>
<connect gate="A" pin="DB26" pad="40"/>
<connect gate="A" pin="DB27" pad="41"/>
<connect gate="A" pin="DB28" pad="42"/>
<connect gate="A" pin="DB29" pad="43"/>
<connect gate="A" pin="DB3" pad="6"/>
<connect gate="A" pin="DB30" pad="44"/>
<connect gate="A" pin="DB31" pad="45"/>
<connect gate="A" pin="DB4" pad="7"/>
<connect gate="A" pin="DB5" pad="8"/>
<connect gate="A" pin="DB6" pad="10"/>
<connect gate="A" pin="DB7" pad="11"/>
<connect gate="A" pin="DB8" pad="13"/>
<connect gate="A" pin="DB9" pad="14"/>
<connect gate="A" pin="ERR" pad="2"/>
<connect gate="A" pin="MERR" pad="1"/>
<connect gate="A" pin="OECB" pad="24"/>
<connect gate="A" pin="OEDB" pad="9"/>
<connect gate="A" pin="S0" pad="46"/>
<connect gate="A" pin="S1" pad="47"/>
<connect gate="P" pin="GND@1" pad="12"/>
<connect gate="P" pin="GND@2" pad="37"/>
<connect gate="P" pin="VCC" pad="48"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*635" prefix="IC">
<description>32-bit &lt;b&gt;EDAC&lt;/b&gt; error detection and correction</description>
<gates>
<gate name="A" symbol="74635"/>
<gate name="P" symbol="PWR2GND"/>
</gates>
<devices>
<device name="JD" package="DIL48">
<connects>
<connect gate="A" pin="CB0" pad="28"/>
<connect gate="A" pin="CB1" pad="27"/>
<connect gate="A" pin="CB2" pad="26"/>
<connect gate="A" pin="CB3" pad="25"/>
<connect gate="A" pin="CB4" pad="23"/>
<connect gate="A" pin="CB5" pad="22"/>
<connect gate="A" pin="CB6" pad="21"/>
<connect gate="A" pin="DB0" pad="3"/>
<connect gate="A" pin="DB1" pad="4"/>
<connect gate="A" pin="DB10" pad="15"/>
<connect gate="A" pin="DB11" pad="16"/>
<connect gate="A" pin="DB12" pad="17"/>
<connect gate="A" pin="DB13" pad="18"/>
<connect gate="A" pin="DB14" pad="19"/>
<connect gate="A" pin="DB15" pad="20"/>
<connect gate="A" pin="DB16" pad="29"/>
<connect gate="A" pin="DB17" pad="30"/>
<connect gate="A" pin="DB18" pad="31"/>
<connect gate="A" pin="DB19" pad="32"/>
<connect gate="A" pin="DB2" pad="5"/>
<connect gate="A" pin="DB20" pad="33"/>
<connect gate="A" pin="DB21" pad="34"/>
<connect gate="A" pin="DB22" pad="35"/>
<connect gate="A" pin="DB23" pad="36"/>
<connect gate="A" pin="DB24" pad="38"/>
<connect gate="A" pin="DB25" pad="39"/>
<connect gate="A" pin="DB26" pad="40"/>
<connect gate="A" pin="DB27" pad="41"/>
<connect gate="A" pin="DB28" pad="42"/>
<connect gate="A" pin="DB29" pad="43"/>
<connect gate="A" pin="DB3" pad="6"/>
<connect gate="A" pin="DB30" pad="44"/>
<connect gate="A" pin="DB31" pad="45"/>
<connect gate="A" pin="DB4" pad="7"/>
<connect gate="A" pin="DB5" pad="8"/>
<connect gate="A" pin="DB6" pad="10"/>
<connect gate="A" pin="DB7" pad="11"/>
<connect gate="A" pin="DB8" pad="13"/>
<connect gate="A" pin="DB9" pad="14"/>
<connect gate="A" pin="ERR" pad="2"/>
<connect gate="A" pin="MERR" pad="1"/>
<connect gate="A" pin="OECB" pad="24"/>
<connect gate="A" pin="OEDB" pad="9"/>
<connect gate="A" pin="S0" pad="46"/>
<connect gate="A" pin="S1" pad="47"/>
<connect gate="P" pin="GND@1" pad="12"/>
<connect gate="P" pin="GND@2" pad="37"/>
<connect gate="P" pin="VCC" pad="48"/>
</connects>
<technologies>
<technology name="ALS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*870" prefix="IC">
<description>2 x 16 &lt;b&gt;REGISTER&lt;/b&gt;, 4 bit each</description>
<gates>
<gate name="A" symbol="74870"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="NT" package="DIL24-3">
<connects>
<connect gate="A" pin="1A0" pad="2"/>
<connect gate="A" pin="1A1" pad="3"/>
<connect gate="A" pin="1A2" pad="4"/>
<connect gate="A" pin="1A3" pad="5"/>
<connect gate="A" pin="1W" pad="6"/>
<connect gate="A" pin="2A0" pad="19"/>
<connect gate="A" pin="2A1" pad="20"/>
<connect gate="A" pin="2A2" pad="21"/>
<connect gate="A" pin="2A3" pad="22"/>
<connect gate="A" pin="2W" pad="18"/>
<connect gate="A" pin="DQA1" pad="8"/>
<connect gate="A" pin="DQA2" pad="9"/>
<connect gate="A" pin="DQA3" pad="10"/>
<connect gate="A" pin="DQA4" pad="11"/>
<connect gate="A" pin="DQB1" pad="13"/>
<connect gate="A" pin="DQB2" pad="14"/>
<connect gate="A" pin="DQB3" pad="15"/>
<connect gate="A" pin="DQB4" pad="16"/>
<connect gate="A" pin="S0" pad="1"/>
<connect gate="A" pin="S1" pad="23"/>
<connect gate="A" pin="S2" pad="7"/>
<connect gate="A" pin="S3" pad="17"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*871" prefix="IC">
<description>2 x 16 &lt;b&gt;REGISTER&lt;/b&gt;, 4 bit each</description>
<gates>
<gate name="A" symbol="74871"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL28-3">
<connects>
<connect gate="A" pin="1A0" pad="4"/>
<connect gate="A" pin="1A1" pad="5"/>
<connect gate="A" pin="1A2" pad="6"/>
<connect gate="A" pin="1A3" pad="7"/>
<connect gate="A" pin="1W" pad="8"/>
<connect gate="A" pin="2A0" pad="21"/>
<connect gate="A" pin="2A1" pad="22"/>
<connect gate="A" pin="2A2" pad="23"/>
<connect gate="A" pin="2A3" pad="24"/>
<connect gate="A" pin="2W" pad="20"/>
<connect gate="A" pin="DA1" pad="1"/>
<connect gate="A" pin="DA2" pad="2"/>
<connect gate="A" pin="DA3" pad="26"/>
<connect gate="A" pin="DA4" pad="27"/>
<connect gate="A" pin="DQB1" pad="15"/>
<connect gate="A" pin="DQB2" pad="16"/>
<connect gate="A" pin="DQB3" pad="17"/>
<connect gate="A" pin="DQB4" pad="18"/>
<connect gate="A" pin="QA1" pad="10"/>
<connect gate="A" pin="QA2" pad="11"/>
<connect gate="A" pin="QA3" pad="12"/>
<connect gate="A" pin="QA4" pad="13"/>
<connect gate="A" pin="S0" pad="3"/>
<connect gate="A" pin="S1" pad="25"/>
<connect gate="A" pin="S2" pad="9"/>
<connect gate="A" pin="S3" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="AS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*16" prefix="IC">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;, open collector, high-voltage</description>
<gates>
<gate name="A" symbol="7405"/>
<gate name="B" symbol="7405"/>
<gate name="C" symbol="7405"/>
<gate name="D" symbol="7405"/>
<gate name="E" symbol="7405"/>
<gate name="F" symbol="7405"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*17" prefix="IC">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;, open collector, high-voltage</description>
<gates>
<gate name="A" symbol="7405"/>
<gate name="B" symbol="7405"/>
<gate name="C" symbol="7405"/>
<gate name="D" symbol="7405"/>
<gate name="E" symbol="7405"/>
<gate name="F" symbol="7405"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="1"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="4"/>
<connect gate="C" pin="I" pad="5"/>
<connect gate="C" pin="O" pad="6"/>
<connect gate="D" pin="I" pad="9"/>
<connect gate="D" pin="O" pad="8"/>
<connect gate="E" pin="I" pad="11"/>
<connect gate="E" pin="O" pad="10"/>
<connect gate="F" pin="I" pad="13"/>
<connect gate="F" pin="O" pad="12"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*19" prefix="IC">
<description>Hex schmitt trigger &lt;b&gt;INVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="7414"/>
<gate name="B" symbol="7414"/>
<gate name="C" symbol="7414"/>
<gate name="D" symbol="7414"/>
<gate name="E" symbol="7414"/>
<gate name="F" symbol="7414"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I" pad="11"/>
<connect gate="B" pin="O" pad="10"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I" pad="1"/>
<connect gate="D" pin="O" pad="2"/>
<connect gate="E" pin="I" pad="3"/>
<connect gate="E" pin="O" pad="4"/>
<connect gate="F" pin="I" pad="5"/>
<connect gate="F" pin="O" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="I" pad="13"/>
<connect gate="A" pin="O" pad="12"/>
<connect gate="B" pin="I" pad="11"/>
<connect gate="B" pin="O" pad="10"/>
<connect gate="C" pin="I" pad="9"/>
<connect gate="C" pin="O" pad="8"/>
<connect gate="D" pin="I" pad="1"/>
<connect gate="D" pin="O" pad="2"/>
<connect gate="E" pin="I" pad="3"/>
<connect gate="E" pin="O" pad="4"/>
<connect gate="F" pin="I" pad="5"/>
<connect gate="F" pin="O" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74S51" prefix="IC">
<description>&lt;b&gt;AND OR INVERTER&lt;/b&gt; gates/for LS-type see &lt;a href=DEVICE:74*51&gt;74*51&lt;/a&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G$1" symbol="74S51"/>
</gates>
<devices>
<device name="FK" package="LCC20">
<connects>
<connect gate="G$1" pin="1A" pad="2"/>
<connect gate="G$1" pin="1B" pad="19"/>
<connect gate="G$1" pin="1C" pad="13"/>
<connect gate="G$1" pin="1D" pad="14"/>
<connect gate="G$1" pin="1Y" pad="12"/>
<connect gate="G$1" pin="2A" pad="3"/>
<connect gate="G$1" pin="2B" pad="4"/>
<connect gate="G$1" pin="2C" pad="6"/>
<connect gate="G$1" pin="2D" pad="8"/>
<connect gate="G$1" pin="2Y" pad="9"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N" package="DIL14">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1B" pad="13"/>
<connect gate="G$1" pin="1C" pad="9"/>
<connect gate="G$1" pin="1D" pad="10"/>
<connect gate="G$1" pin="1Y" pad="8"/>
<connect gate="G$1" pin="2A" pad="2"/>
<connect gate="G$1" pin="2B" pad="3"/>
<connect gate="G$1" pin="2C" pad="4"/>
<connect gate="G$1" pin="2D" pad="5"/>
<connect gate="G$1" pin="2Y" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="G$1" pin="1A" pad="1"/>
<connect gate="G$1" pin="1B" pad="13"/>
<connect gate="G$1" pin="1C" pad="9"/>
<connect gate="G$1" pin="1D" pad="10"/>
<connect gate="G$1" pin="1Y" pad="8"/>
<connect gate="G$1" pin="2A" pad="2"/>
<connect gate="G$1" pin="2B" pad="3"/>
<connect gate="G$1" pin="2C" pad="4"/>
<connect gate="G$1" pin="2D" pad="5"/>
<connect gate="G$1" pin="2Y" pad="6"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74HC*73" prefix="IC">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="A" symbol="74HC73"/>
<gate name="B" symbol="74HC73"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="!Q" pad="13"/>
<connect gate="A" pin="CP" pad="1"/>
<connect gate="A" pin="J" pad="14"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="Q" pad="12"/>
<connect gate="A" pin="R" pad="2"/>
<connect gate="B" pin="!Q" pad="8"/>
<connect gate="B" pin="CP" pad="5"/>
<connect gate="B" pin="J" pad="7"/>
<connect gate="B" pin="K" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="B" pin="R" pad="6"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="T"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="!Q" pad="13"/>
<connect gate="A" pin="CP" pad="1"/>
<connect gate="A" pin="J" pad="14"/>
<connect gate="A" pin="K" pad="3"/>
<connect gate="A" pin="Q" pad="12"/>
<connect gate="A" pin="R" pad="2"/>
<connect gate="B" pin="!Q" pad="8"/>
<connect gate="B" pin="CP" pad="5"/>
<connect gate="B" pin="J" pad="7"/>
<connect gate="B" pin="K" pad="10"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="B" pin="R" pad="6"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="T"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*47" prefix="IC">
<description>BCD to seven segment &lt;b&gt;DECODER/DRIVER&lt;/b&gt;&lt;p&gt;
Source: http://www.ee.washington.edu/stores/DataSheets/74ls/74ls47.pdf</description>
<gates>
<gate name="G$2" symbol="PWRN"/>
<gate name="G$1" symbol="7447"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="A" pad="13"/>
<connect gate="G$1" pin="B" pad="12"/>
<connect gate="G$1" pin="BI/RBO" pad="4"/>
<connect gate="G$1" pin="C" pad="11"/>
<connect gate="G$1" pin="D" pad="10"/>
<connect gate="G$1" pin="E" pad="9"/>
<connect gate="G$1" pin="F" pad="15"/>
<connect gate="G$1" pin="G" pad="14"/>
<connect gate="G$1" pin="IA" pad="7"/>
<connect gate="G$1" pin="IB" pad="1"/>
<connect gate="G$1" pin="IC" pad="2"/>
<connect gate="G$1" pin="ID" pad="6"/>
<connect gate="G$1" pin="LT" pad="3"/>
<connect gate="G$1" pin="RBI" pad="5"/>
<connect gate="G$2" pin="GND" pad="8"/>
<connect gate="G$2" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*191" prefix="IC">
<description>Synchronous &lt;b&gt; UP/DOWN COUNTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="74190-1"/>
<gate name="P" symbol="PWRN-1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CTE" pad="4"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="D/!U" pad="5"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="MX/MN" pad="12"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name=""/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
</technologies>
</device>
<device name="NS" package="SO16NS">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CTE" pad="4"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="D/!U" pad="5"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="MX/MN" pad="12"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
<device name="D" package="SO16D">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CTE" pad="4"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="D/!U" pad="5"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="MX/MN" pad="12"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
<device name="PW" package="SO16PW">
<connects>
<connect gate="A" pin="A" pad="15"/>
<connect gate="A" pin="B" pad="1"/>
<connect gate="A" pin="C" pad="10"/>
<connect gate="A" pin="CLK" pad="14"/>
<connect gate="A" pin="CTE" pad="4"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="D/!U" pad="5"/>
<connect gate="A" pin="LD" pad="11"/>
<connect gate="A" pin="MX/MN" pad="12"/>
<connect gate="A" pin="QA" pad="3"/>
<connect gate="A" pin="QB" pad="2"/>
<connect gate="A" pin="QC" pad="6"/>
<connect gate="A" pin="QD" pad="7"/>
<connect gate="A" pin="RCO" pad="13"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74C922" prefix="IC">
<description>&lt;b&gt;16-Key Encoder&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/ds/MM/MM54C922.pdf#page=1</description>
<gates>
<gate name="G$1" symbol="74922"/>
<gate name="P" symbol="PWRN-2"/>
</gates>
<devices>
<device name="N" package="DIL18">
<connects>
<connect gate="G$1" pin="!OE" pad="13"/>
<connect gate="G$1" pin="DATA_AV" pad="12"/>
<connect gate="G$1" pin="KBM" pad="6"/>
<connect gate="G$1" pin="OSC" pad="5"/>
<connect gate="G$1" pin="OUTA" pad="17"/>
<connect gate="G$1" pin="OUTB" pad="16"/>
<connect gate="G$1" pin="OUTC" pad="15"/>
<connect gate="G$1" pin="OUTD" pad="14"/>
<connect gate="G$1" pin="X1" pad="11"/>
<connect gate="G$1" pin="X2" pad="10"/>
<connect gate="G$1" pin="X3" pad="8"/>
<connect gate="G$1" pin="X4" pad="7"/>
<connect gate="G$1" pin="Y1" pad="1"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="3"/>
<connect gate="G$1" pin="Y4" pad="4"/>
<connect gate="P" pin="GND" pad="9"/>
<connect gate="P" pin="VCC" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SO20W">
<connects>
<connect gate="G$1" pin="!OE" pad="14"/>
<connect gate="G$1" pin="DATA_AV" pad="13"/>
<connect gate="G$1" pin="KBM" pad="7"/>
<connect gate="G$1" pin="OSC" pad="6"/>
<connect gate="G$1" pin="OUTA" pad="19"/>
<connect gate="G$1" pin="OUTB" pad="18"/>
<connect gate="G$1" pin="OUTC" pad="17"/>
<connect gate="G$1" pin="OUTD" pad="16"/>
<connect gate="G$1" pin="X1" pad="12"/>
<connect gate="G$1" pin="X2" pad="11"/>
<connect gate="G$1" pin="X3" pad="8"/>
<connect gate="G$1" pin="X4" pad="9"/>
<connect gate="G$1" pin="Y1" pad="1"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="3"/>
<connect gate="G$1" pin="Y4" pad="4"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74C923" prefix="IC">
<description>&lt;b&gt;20-Key Encoder&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/ds/MM/MM54C922.pdf#page=1</description>
<gates>
<gate name="G$1" symbol="74923"/>
<gate name="P" symbol="PWRN-2"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="G$1" pin="!OE" pad="14"/>
<connect gate="G$1" pin="DATA_AV" pad="13"/>
<connect gate="G$1" pin="KBM" pad="7"/>
<connect gate="G$1" pin="OSC" pad="6"/>
<connect gate="G$1" pin="OUTA" pad="19"/>
<connect gate="G$1" pin="OUTB" pad="18"/>
<connect gate="G$1" pin="OUTC" pad="17"/>
<connect gate="G$1" pin="OUTD" pad="16"/>
<connect gate="G$1" pin="OUTE" pad="15"/>
<connect gate="G$1" pin="X1" pad="12"/>
<connect gate="G$1" pin="X2" pad="11"/>
<connect gate="G$1" pin="X3" pad="9"/>
<connect gate="G$1" pin="X4" pad="8"/>
<connect gate="G$1" pin="Y1" pad="1"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="3"/>
<connect gate="G$1" pin="Y4" pad="4"/>
<connect gate="G$1" pin="Y5" pad="5"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SO20W">
<connects>
<connect gate="G$1" pin="!OE" pad="14"/>
<connect gate="G$1" pin="DATA_AV" pad="13"/>
<connect gate="G$1" pin="KBM" pad="7"/>
<connect gate="G$1" pin="OSC" pad="6"/>
<connect gate="G$1" pin="OUTA" pad="19"/>
<connect gate="G$1" pin="OUTB" pad="18"/>
<connect gate="G$1" pin="OUTC" pad="17"/>
<connect gate="G$1" pin="OUTD" pad="16"/>
<connect gate="G$1" pin="OUTE" pad="15"/>
<connect gate="G$1" pin="X1" pad="12"/>
<connect gate="G$1" pin="X2" pad="11"/>
<connect gate="G$1" pin="X3" pad="9"/>
<connect gate="G$1" pin="X4" pad="8"/>
<connect gate="G$1" pin="Y1" pad="1"/>
<connect gate="G$1" pin="Y2" pad="2"/>
<connect gate="G$1" pin="Y3" pad="3"/>
<connect gate="G$1" pin="Y4" pad="4"/>
<connect gate="G$1" pin="Y5" pad="5"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
