<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.2">
<drawing>
<library>
<description>&lt;b&gt;Analog Devices Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PQFP240">
<description>&lt;b&gt;PLASTIC QUAD FLAT PACK&lt;/b&gt;</description>
</package>
<package name="PQFP208">
<description>&lt;b&gt;PLASTIC QUAD FLAT PACK&lt;/b&gt;</description>
</package>
<package name="TQFP100">
<description>&lt;b&gt;THIN QUAD FLAT PACK&lt;/b&gt;</description>
</package>
<package name="SO8-COOL">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="PQFP52">
<description>&lt;b&gt;PLASTIC QUAD FLAT PACK&lt;/b&gt;</description>
</package>
<package name="AD102">
<description>&lt;b&gt;8 lead Package&lt;/b&gt;</description>
</package>
<package name="AD104">
<description>&lt;b&gt;8 lead Package&lt;/b&gt;</description>
</package>
<package name="PLCC28S">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;</description>
</package>
<package name="SO8">
<description>&lt;b&gt;8-Lead Small Outline IC&lt;/b&gt; (SO-8)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf</description>
</package>
<package name="LCC20">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;</description>
</package>
<package name="TO100">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="SOIC16N">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="MICROSOIC10">
<description>&lt;b&gt;10-Lead microSOIC&lt;/b&gt;&lt;p&gt;
(RM-10) 10-µSOIC</description>
</package>
<package name="LQFP100">
<description>&lt;b&gt;100-Lead Metric Thin Plastic Quad Flatpack&lt;/b&gt;</description>
</package>
<package name="SO10">
<description>&lt;b&gt;10-Lead Mini_SO Package&lt;/b&gt;&lt;p&gt;
(RM-10)</description>
</package>
<package name="MBGA225">
<description>&lt;b&gt;Micro Ball Grid Aray 225 &lt;/b&gt;</description>
</package>
<package name="TSSOP28">
<description>&lt;b&gt;28-Lead TSSOP Package&lt;/b&gt;&lt;p&gt;
RU-28</description>
</package>
<package name="LQFP80">
<description>&lt;b&gt;80 Lead LQFP_ED (SQ-80) (ST-80)&lt;/b&gt;&lt;p&gt;
Source: www.analog.com .. AD9852_b.pdf</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="LCC8">
<description>&lt;b&gt;8-Terminal Ceramic Leadless Chip Carrier [LCC] (E-8)&lt;/b&gt;&lt;p&gt;
Source: www.analog.com/UploadedFiles/Packages/189346426E_8.pdf</description>
</package>
<package name="PLCC20">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;&lt;p&gt;IPC standard</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="PQFP44">
<description>&lt;B&gt;Plastic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="BGA_160">
<description>&lt;b&gt;160-Ball Mini-BGA (BC-160)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp&lt;/i&gt;&lt;br&gt;
Source: www.analog.com .. 33260205658992ADSP_BF533_mbga.bsdl</description>
</package>
<package name="LQFP176-1">
<description>&lt;b&gt;176-Lead Metric Thin Plastic Quad Flatpack&lt;/b&gt;&lt;p&gt;
Source: www.analog.com .. 144127970ADSP_BF531_2_3_a.pdf</description>
</package>
<package name="BGA_169">
<description>&lt;b&gt;169-Ball Plastic Ball Grid Array&lt;/b&gt; (B-169)&lt;p&gt;
Source: www.analog.com .. 144127970ADSP_BF531_2_3_a.pdf</description>
</package>
<package name="LFCSP24">
<description>&lt;b&gt;24-Lead Lead Frame Chip Scale Package&lt;/b&gt;&lt;p&gt;
4 mm × 4 mm (CP-24)&lt;br&gt;
Source: www.analog.com .. 3832984220209AD8133_0.pdf</description>
</package>
<package name="MBGA_160">
<description>&lt;b&gt;MBGA 160&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 8&lt;/i&gt;&lt;br&gt;
Source: 33170285923617ADSP_BF531_mbga.bsdl</description>
</package>
<package name="BGA_208">
<description>&lt;b&gt;208-Ball Sparse Mini-BGA&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 8&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/90140778ADSP_BF536_7_prd.pdf&lt;br&gt;
Source2: BSDL_br.txt as Email: &amp;lt;adi-germany@analog.com&amp;gt;</description>
</package>
<package name="MINI-BGA-182">
<description>&lt;b&gt;182-Ball Mini-BGA&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/90140778ADSP_BF536_7_prd.pdf</description>
</package>
<package name="LFCSP16">
<description>&lt;b&gt;16-Terminal Leadless Frame Chip Scale Package [LFCSP] (CP)&lt;/b&gt;&lt;p&gt;
Source: Analog Devices .. 780914713ADD8704_0.pdf</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;14-Lead Thin Shrink Small Outline Package [TSSOP]&lt;/b&gt;&lt;p&gt;
Source: Analog Devices .. 780914713ADD8704_0.pdf</description>
</package>
<package name="LFCSP64">
<description>&lt;b&gt;64-Lead Lead Frame Chip Scale Package [LFCSP] CP-64-1&lt;/b&gt; 9 x 9 mm Body&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Packages/40887351787287CP_64_1.pdf</description>
</package>
<package name="PBGA_B260">
<description>&lt;b&gt;ADSP_21535.bsdl&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 11&lt;/i&gt;&lt;br&gt;
Source: ADSP_21535.bsdl&lt;br&gt;
http://www.analog.com/UploadedFiles/Data_Sheets/744511807ADSP_BF535_a.pdf</description>
</package>
<package name="PBGA196">
<description>&lt;b&gt;196-Lead PBGA&lt;/b&gt; (BC-196)&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 11&lt;/i&gt;&lt;br&gt;
Source: 90033586AD6624A.bsdl.txt&lt;br&gt;
http://www.analog.com/UploadedFiles/Data_Sheets/171976900AD6624A_0.pdf</description>
</package>
<package name="TSSOP38">
<description>&lt;b&gt;38-Lead Thin Shrink Small Outline Package&lt;/b&gt; [TSSOP] RU-38&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Packages/415413609854197792024125RU38.pdf&lt;br&gt;
COMPLIANT TO JEDEC STANDARDS MS-153BD-1</description>
</package>
<package name="LFCSP40">
<description>&lt;b&gt;40-Lead Frame Chip Scale Package [LFCSP_VQ]&lt;/b&gt; 6 mm x 6 mm Body, Very Thin Quad (CP-40)&lt;p&gt;
COMPLIANT TO JEDEC STANDARDS MO-220-VJJD-2&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/288945048AD7C7019_20_1_2_4_5_6_7_0.pdf</description>
</package>
<package name="QFP64_SOT393">
<description>&lt;b&gt;Plastic Quad Flat Package SOT393-1/-2&lt;/b&gt; 64 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="LQFP_ST-80-1">
<description>&lt;b&gt;80-Lead Low Profile Quad Flat Package&lt;/b&gt; (ST-80-1)&lt;p&gt;
COMPLIANT TO JEDEC STANDARDS MS-026-BDD&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/288945048AD7C7019_20_1_2_4_5_6_7_0.pdf</description>
</package>
<package name="LQFP-ST-64-2">
<description>&lt;b&gt;64-Lead Low Profile Quad Flat Package [LQFP] (ST-64-2)&lt;/b&gt;&lt;p&gt;
COMPLIANT TO JEDEC STANDARDS MS-026-BCD&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/288945048AD7C7019_20_1_2_4_5_6_7_0.pdf</description>
</package>
<package name="MSOP08">
<description>&lt;b&gt;8-Lead micro SO&lt;/b&gt; (RM-8)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf</description>
</package>
<package name="LFCSP32">
<description>&lt;b&gt;32-Lead Frame Chip Scale Package [LFCSP_VQ]&lt;/b&gt; 5 mm × 5 mm Very Thin Quad (CP-32-3&lt;p&gt;
COMPLIANT TO JEDEC STANDARDS MO-220-VHHD-2&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/762180021AD7142_42_1_prd.pdf</description>
</package>
<package name="MSOP10">
<description>&lt;b&gt;10-Lead Mini Small Outline Package [MSOP]&lt;/b&gt; (RM-10)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/35641221898805SSM2167_b.pdf&lt;br&gt;
COMPLIANT TO JEDEC STANDARDS MO-187BA</description>
</package>
<package name="MPBGA256">
<description>&lt;b&gt;MBGA265&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 13&lt;/i&gt;&lt;br&gt;
Source: 37918753ADSP_BF561_256_MBGA_rev0_3.bsdl</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;5-Lead Small Outline Transistor&lt;/b&gt; Package SOT-23&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/346131962AD8067_a.pdf</description>
</package>
<package name="SO24R">
<description>&lt;b&gt;24-Lead Wide Body SOIC&lt;/b&gt; (R-24)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/39677768AD7714_c.pdf</description>
</package>
<package name="SSOP28">
<description>&lt;b&gt;28-Lead Shrink Small Outline Package SSOP&lt;/b&gt; (RS-28)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/39677768AD7714_c.pdf</description>
</package>
<package name="TSSOP24">
<description>&lt;b&gt;24-Lead Thin Shrink Small Outline Package TSSOP&lt;/b&gt; (RU-24)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/39677768AD7714_c.pdf</description>
</package>
<package name="SO-16W">
<description>&lt;b&gt;16-Lead (Wide Body) Small Outline Package&lt;/b&gt; (R-16)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/409317160AD421_c.pdf</description>
</package>
<package name="QFP-7X7-48">
<description>&lt;b&gt;TQFP48&lt;/b&gt; 7x7&lt;p&gt;
Thin Plastic Quad Flat Package, Exposed Pad, TQFP/EP&lt;br&gt;
Source: www.analog.com/UploadedFiles/Data_Sheets/33830397585263AD9859_0.pdf</description>
</package>
<package name="LFCSP48">
<description>&lt;b&gt;Lead Frame Chip Scale Package&lt;/b&gt; LFCSP CP-48&lt;p&gt;
COMPLIANT TO JEDEC STANDARDS MO-220-VKKD-2&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/39780344872292AD7651_0.pdf</description>
</package>
<package name="LFCSP_VD08">
<description>&lt;b&gt;8-Lead Lead Frame Chip Scale Package [LFCSP_VD]&lt;/b&gt;&lt;p&gt;
2 mm × 3 mm Body, Very Thin, Dual Lead CP-8-1&lt;br&gt;
Source: AD8353.pdf</description>
</package>
<package name="BP-256">
<description>&lt;b&gt;256-Ball Gridd Array&lt;/b&gt;, Thermally Enhanced [BGA_ED]&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 26&lt;/i&gt;&lt;br&gt;
Source: 17303025021367_256ballSBGA_bsdl_PrA_0106.txt&lt;br&gt;
http://www.analog.com/static/imported-files/packages/287254833BP_256.pdf</description>
</package>
<package name="LQFP208">
<description>&lt;b&gt;LQFP208&lt;/b&gt;&lt;p&gt;
COMPLIANT TO JEDEC STANDARDS MS-026-BJB-HD&lt;br&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 26&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADSP-21367_21368_21369.pdf&lt;br&gt;
71207126721367_208pinMQFP_bsdl_PrA_0106.txt</description>
</package>
<package name="LGA16">
<description>&lt;b&gt;16-Terminal Land Grid Array [LGA]&lt;/b&gt; (CC-16-2)&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADIS16209.pdf</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;16-Lead Thin Shrink Small Outline Package&lt;/b&gt; [TSSOP] (RU-16)&lt;p&gt;
Source: 8x ADG1408_1409.pdf</description>
</package>
<package name="QSOP16">
<description>&lt;b&gt;16-Lead Shrink Small Outline Package&lt;/b&gt; QSOP (RQ-16)&lt;p&gt;
Source: ADG658_659.pdf</description>
</package>
<package name="SO14">
<description>&lt;b&gt;14-Lead Narrow-Body SOIC&lt;/b&gt; (SO-14)&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/SSM2166.pdf</description>
</package>
<package name="SO-28R">
<description>&lt;B&gt;R-28 (S-Suffix) 28-Lead Wide-Body SO&lt;/b&gt; SOL-28&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1877.pdf</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="AD210">
<description>Source: http://www.analog.com/static/imported-files/data_sheets/AD210.pdf</description>
</package>
<package name="AD215">
<description>&lt;b&gt;AD215 SIP PACKAGE&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD215.pdf</description>
</package>
<package name="H08">
<description>&lt;b&gt;8-Lead Metal Can TO-99&lt;/b&gt; (H-8)&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD711.pdf</description>
</package>
<package name="SOIC16R">
<description>&lt;b&gt;16-Lead SOIC (R) Package&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD745.pdf</description>
</package>
<package name="SOIC20R">
<description>&lt;b&gt;20-LeadStandard Small Outline Package SOIC Wide Body (R-20)&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD811.pdf</description>
</package>
<package name="SC70-5">
<description>&lt;b&gt;5-Lead Thin Shrink Small Outline Transistor Package&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8519_8529.pdf</description>
</package>
<package name="TSSOP8">
<description>&lt;b&gt;8-Lead Thin Shrink Small Outline Package &lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8541_8542_8544.pdf</description>
</package>
<package name="LFCSP8">
<description>&lt;b&gt;8-Lead Lead Frame Chip Scale Package&lt;/b&gt; LFCSP_VD 3 mm × 3 mm Body, Very Thin, Dual Lead&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8597_8599.pdf</description>
</package>
<package name="LFCSP8_CP">
<description>&lt;b&gt;8-Lead Lead Frame Chip Scale Package&lt;/b&gt; LFCSP_WD 2 mm × 2 mm Body, Very Very Thin, Dual Lead&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4075-2.pdf</description>
</package>
<package name="SC70-6">
<description>&lt;b&gt;6-Lead Thin Shrink Small Outline Transistor Package SC70&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4853-1_4853-2_4853-3.pdf</description>
</package>
<package name="BGA_256">
<description>&lt;b&gt;256-Ball Ball Grid Array, Thermally Enhanced&lt;/b&gt; BGA_ED&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: 78445023821368_256ballSBGA_bsdl_PrA_0206.txt&lt;br&gt;
http://www.analog.com/static/imported-files/data_sheets/ADSP-21367_21368_21369.pdf</description>
</package>
<package name="BGA_324_CSP">
<description>&lt;b&gt;ADSP_21462W_324_CSPBGA_bsdl&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: ADSP_21462W_324_CSPBGA_bsdl.txt</description>
</package>
<package name="BGA_CB11">
<description>&lt;b&gt;11-Ball, Backside-Coated, Wafer Level Chip Scale Package&lt;/b&gt; WLCSP&lt;p&gt;
CB-11-1&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8235.pdf</description>
</package>
<package name="MQFP52">
<description>&lt;b&gt;52-Lead Metric Quad Flat Package MQFP&lt;/b&gt; S-52-2&lt;p&gt;
COMPLIANT TO JEDEC STANDARDS MO-112-AC-1&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADUC845_847_848.pdf</description>
</package>
<package name="LFCSP56">
<description>&lt;b&gt;56-Lead Frame Chip Scale Package LFCSP&lt;/b&gt; 8 mm × 8 mm Body, Very Thin Quad (CP-56)&lt;p&gt;
COMPLIANT TO JEDEC STANDARDS MO-220-VLLD-2&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADUC845_847_848.pdf</description>
</package>
</packages>
<symbols>
<symbol name="SP21065L">
<pin name="RFS0"/>
<pin name="RCLK0"/>
<pin name="DR0A" direction="in"/>
<pin name="DR0B" direction="in"/>
<pin name="TFS0"/>
<pin name="TCLK0"/>
<pin name="DT0A" direction="out"/>
<pin name="DT0B" direction="out"/>
<pin name="RFS1"/>
<pin name="RCLK1"/>
<pin name="DR1A" direction="in"/>
<pin name="DR1B" direction="in"/>
<pin name="TFS1"/>
<pin name="TCLK1"/>
<pin name="CAS/" direction="hiz"/>
<pin name="SDWE/" direction="hiz"/>
<pin name="DQM/" direction="hiz"/>
<pin name="SDCKE" direction="hiz"/>
<pin name="SDA10" direction="hiz"/>
<pin name="DMAG1/" direction="hiz"/>
<pin name="DMAG2/" direction="hiz"/>
<pin name="HBG/"/>
<pin name="BMSTR" direction="out"/>
<pin name="CS/" direction="in"/>
<pin name="SBTS/" direction="in"/>
<pin name="WR/" direction="hiz"/>
<pin name="RD/" direction="hiz"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="DATA16"/>
<pin name="DATA17"/>
<pin name="DATA18"/>
<pin name="DATA19"/>
<pin name="DATA20"/>
<pin name="DATA21"/>
<pin name="DATA22"/>
<pin name="DATA23"/>
<pin name="DATA24"/>
<pin name="DATA25"/>
<pin name="DATA26"/>
<pin name="DATA27"/>
<pin name="ADDR0"/>
<pin name="ADDR1"/>
<pin name="ADDR2"/>
<pin name="ADDR3"/>
<pin name="ADDR4"/>
<pin name="ADDR5"/>
<pin name="ADDR6"/>
<pin name="ADDR7"/>
<pin name="ADDR8"/>
<pin name="ADDR9"/>
<pin name="ADDR10"/>
<pin name="ADDR11"/>
<pin name="ADDR12"/>
<pin name="ADDR13"/>
<pin name="ADDR14"/>
<pin name="ADDR15"/>
<pin name="ADDR16"/>
<pin name="ADDR17"/>
<pin name="ADDR18"/>
<pin name="ADDR19"/>
<pin name="ADDR20"/>
<pin name="ADDR21"/>
<pin name="ADDR22"/>
<pin name="DATA28"/>
<pin name="DATA29"/>
<pin name="DATA30"/>
<pin name="DATA31"/>
<pin name="ADDR23"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="FLAG4"/>
<pin name="FLAG5"/>
<pin name="FLAG6"/>
<pin name="FLAG7"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="EMU/" direction="out"/>
<pin name="DT1A" direction="out"/>
<pin name="DT1B" direction="out"/>
<pin name="PWM_EVENT0"/>
<pin name="PWM_EVENT1"/>
<pin name="BR1/"/>
<pin name="BR2/"/>
<pin name="CLKIN" direction="in"/>
<pin name="XTAL/" direction="out"/>
<pin name="SDCLK1" direction="hiz"/>
<pin name="SDCLK0" direction="hiz"/>
<pin name="DMAR1/" direction="in"/>
<pin name="DMAR2/" direction="in"/>
<pin name="HBR/" direction="in"/>
<pin name="RAS/" direction="hiz"/>
<pin name="REDY/" direction="out"/>
<pin name="SW/" direction="hiz"/>
<pin name="CPA/"/>
<pin name="ACK"/>
<pin name="MS0/" direction="hiz"/>
<pin name="MS1/" direction="hiz"/>
<pin name="MS2/" direction="hiz"/>
<pin name="MS3/" direction="hiz"/>
<pin name="FLAG8"/>
<pin name="FLAG9"/>
<pin name="FLAG10"/>
<pin name="FLAG11"/>
<pin name="TDO" direction="out"/>
<pin name="TRST/" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="BSEL" direction="in"/>
<pin name="BMS/"/>
<pin name="RESET/" direction="in"/>
<pin name="IRQ0/" direction="in"/>
<pin name="IRQ1/" direction="in"/>
<pin name="IRQ2/" direction="in"/>
</symbol>
<symbol name="GND37">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
</symbol>
<symbol name="VCC32">
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="VCC@7" direction="pwr"/>
<pin name="VCC@8" direction="pwr"/>
<pin name="VCC@9" direction="pwr"/>
<pin name="VCC@10" direction="pwr"/>
<pin name="VCC@11" direction="pwr"/>
<pin name="VCC@12" direction="pwr"/>
<pin name="VCC@13" direction="pwr"/>
<pin name="VCC@14" direction="pwr"/>
<pin name="VCC@15" direction="pwr"/>
<pin name="VCC@16" direction="pwr"/>
<pin name="VCC@17" direction="pwr"/>
<pin name="VCC@18" direction="pwr"/>
<pin name="VCC@19" direction="pwr"/>
<pin name="VCC@20" direction="pwr"/>
<pin name="VCC@21" direction="pwr"/>
<pin name="VCC@22" direction="pwr"/>
<pin name="VCC@23" direction="pwr"/>
<pin name="VCC@24" direction="pwr"/>
<pin name="VCC@25" direction="pwr"/>
<pin name="VCC@26" direction="pwr"/>
<pin name="VCC@27" direction="pwr"/>
<pin name="VCC@28" direction="pwr"/>
<pin name="VCC@29" direction="pwr"/>
<pin name="VCC@30" direction="pwr"/>
<pin name="VCC@31" direction="pwr"/>
<pin name="VCC@32" direction="pwr"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="GND31">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
</symbol>
<symbol name="VCC29">
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="VCC@7" direction="pwr"/>
<pin name="VCC@8" direction="pwr"/>
<pin name="VCC@9" direction="pwr"/>
<pin name="VCC@10" direction="pwr"/>
<pin name="VCC@11" direction="pwr"/>
<pin name="VCC@12" direction="pwr"/>
<pin name="VCC@13" direction="pwr"/>
<pin name="VCC@14" direction="pwr"/>
<pin name="VCC@15" direction="pwr"/>
<pin name="VCC@16" direction="pwr"/>
<pin name="VCC@17" direction="pwr"/>
<pin name="VCC@18" direction="pwr"/>
<pin name="VCC@19" direction="pwr"/>
<pin name="VCC@20" direction="pwr"/>
<pin name="VCC@21" direction="pwr"/>
<pin name="VCC@22" direction="pwr"/>
<pin name="VCC@23" direction="pwr"/>
<pin name="VCC@24" direction="pwr"/>
<pin name="VCC@25" direction="pwr"/>
<pin name="VCC@26" direction="pwr"/>
<pin name="VCC@27" direction="pwr"/>
<pin name="VCC@28" direction="pwr"/>
</symbol>
<symbol name="SP21060">
<pin name="RFS0"/>
<pin name="RCLK0"/>
<pin name="DR0" direction="in"/>
<pin name="TFS0"/>
<pin name="TCLK0"/>
<pin name="DT0" direction="out"/>
<pin name="RFS1"/>
<pin name="RCLK1"/>
<pin name="DR1" direction="in"/>
<pin name="TFS1"/>
<pin name="TCLK1"/>
<pin name="DMAG1/" direction="hiz"/>
<pin name="DMAG2/" direction="hiz"/>
<pin name="HBG/"/>
<pin name="CS/" direction="in"/>
<pin name="SBTS/" direction="in"/>
<pin name="WR/_" direction="hiz"/>
<pin name="RD/" direction="hiz"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D16"/>
<pin name="D17"/>
<pin name="D18"/>
<pin name="D19"/>
<pin name="D20"/>
<pin name="D21"/>
<pin name="D22"/>
<pin name="D23"/>
<pin name="D24"/>
<pin name="D25"/>
<pin name="D26"/>
<pin name="D27"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16"/>
<pin name="A17"/>
<pin name="A18"/>
<pin name="A19"/>
<pin name="A20"/>
<pin name="A21"/>
<pin name="A22"/>
<pin name="D28"/>
<pin name="D29"/>
<pin name="D30"/>
<pin name="D31"/>
<pin name="A23"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="EMU/" direction="out"/>
<pin name="DT1" direction="out"/>
<pin name="BR1/"/>
<pin name="BR2/"/>
<pin name="CLKIN" direction="in"/>
<pin name="DMAR1/" direction="in"/>
<pin name="DMAR2/" direction="in"/>
<pin name="HBR/" direction="in"/>
<pin name="REDY/" direction="out"/>
<pin name="SW/" direction="hiz"/>
<pin name="CPA/"/>
<pin name="ACK"/>
<pin name="MS0/" direction="hiz"/>
<pin name="MS1/" direction="hiz"/>
<pin name="MS2/" direction="hiz"/>
<pin name="MS3/" direction="hiz"/>
<pin name="TDO" direction="out"/>
<pin name="TRST/" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="BMS/"/>
<pin name="RESET/" direction="in"/>
<pin name="IRQ0/" direction="in"/>
<pin name="IRQ1/" direction="in"/>
<pin name="IRQ2/" direction="in"/>
<pin name="A24"/>
<pin name="A25"/>
<pin name="A26"/>
<pin name="A27"/>
<pin name="A28"/>
<pin name="A29"/>
<pin name="A30"/>
<pin name="A31"/>
<pin name="D32"/>
<pin name="D33"/>
<pin name="D34"/>
<pin name="D35"/>
<pin name="D36"/>
<pin name="D37"/>
<pin name="D38"/>
<pin name="D39"/>
<pin name="D40"/>
<pin name="D41"/>
<pin name="D42"/>
<pin name="D43"/>
<pin name="D44"/>
<pin name="D45"/>
<pin name="D46"/>
<pin name="D47"/>
<pin name="PAGE" direction="hiz"/>
<pin name="ADRCLK" direction="hiz"/>
<pin name="TIMEXP" direction="out"/>
<pin name="RPBA" direction="in"/>
<pin name="L0DAT0"/>
<pin name="L0DAT1"/>
<pin name="L0DAT2"/>
<pin name="L0DAT3"/>
<pin name="L0CLK"/>
<pin name="L0ACK"/>
<pin name="EBOOT" direction="in"/>
<pin name="LBOOT" direction="in"/>
<pin name="ICSA" direction="out"/>
<pin name="BR3/"/>
<pin name="BR4/"/>
<pin name="BR5/"/>
<pin name="BR6/"/>
<pin name="L1DAT0"/>
<pin name="L1DAT1"/>
<pin name="L1DAT2"/>
<pin name="L1DAT3"/>
<pin name="L1CLK"/>
<pin name="L1ACK"/>
<pin name="L2DAT0"/>
<pin name="L2DAT1"/>
<pin name="L2DAT2"/>
<pin name="L2DAT3"/>
<pin name="L2CLK"/>
<pin name="L2ACK"/>
<pin name="L3DAT0"/>
<pin name="L3DAT1"/>
<pin name="L3DAT2"/>
<pin name="L3DAT3"/>
<pin name="L3CLK"/>
<pin name="L3ACK"/>
<pin name="L4DAT0"/>
<pin name="L4DAT1"/>
<pin name="L4DAT2"/>
<pin name="L4DAT3"/>
<pin name="L4CLK"/>
<pin name="L4ACK"/>
<pin name="L5DAT0"/>
<pin name="L5DAT1"/>
<pin name="L5DAT2"/>
<pin name="L5DAT3"/>
<pin name="L5CLK"/>
<pin name="L5ACK"/>
<pin name="ID2" direction="in"/>
</symbol>
<symbol name="ADP3303">
<pin name="OUT" direction="pas"/>
<pin name="OUT@2" direction="pas"/>
<pin name="NR" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="SC/" direction="in"/>
<pin name="ERR/" direction="oc"/>
<pin name="IN" direction="in"/>
<pin name="IN@1" direction="in"/>
</symbol>
<symbol name="SP21060C">
<pin name="RFS0"/>
<pin name="RCLK0"/>
<pin name="DR0" direction="in"/>
<pin name="TFS0"/>
<pin name="TCLK0"/>
<pin name="DT0" direction="out"/>
<pin name="RFS1"/>
<pin name="RCLK1"/>
<pin name="DR1" direction="in"/>
<pin name="TFS1"/>
<pin name="TCLK1"/>
<pin name="DMAG1/" direction="hiz"/>
<pin name="DMAG2/" direction="hiz"/>
<pin name="HBG/"/>
<pin name="CS/" direction="in"/>
<pin name="SBTS/" direction="in"/>
<pin name="WR/_" direction="hiz"/>
<pin name="RD/" direction="hiz"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="EMU/" direction="out"/>
<pin name="DT1" direction="out"/>
<pin name="BR1/"/>
<pin name="BR2/"/>
<pin name="CLKIN" direction="in"/>
<pin name="DMAR1/" direction="in"/>
<pin name="DMAR2/" direction="in"/>
<pin name="HBR/" direction="in"/>
<pin name="REDY/" direction="out"/>
<pin name="SW/" direction="hiz"/>
<pin name="CPA/"/>
<pin name="ACK"/>
<pin name="MS0/" direction="hiz"/>
<pin name="MS1/" direction="hiz"/>
<pin name="MS2/" direction="hiz"/>
<pin name="MS3/" direction="hiz"/>
<pin name="TDO" direction="out"/>
<pin name="TRST/" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="BMS/"/>
<pin name="RESET/" direction="in"/>
<pin name="IRQ0/" direction="in"/>
<pin name="IRQ1/" direction="in"/>
<pin name="IRQ2/" direction="in"/>
<pin name="PAGE" direction="hiz"/>
<pin name="ADRCLK" direction="hiz"/>
<pin name="TIMEXP" direction="out"/>
<pin name="RPBA" direction="in"/>
<pin name="EBOOT" direction="in"/>
<pin name="LBOOT" direction="in"/>
<pin name="ICSA" direction="out"/>
<pin name="BR3/"/>
<pin name="BR4/"/>
<pin name="BR5/"/>
<pin name="BR6/"/>
<pin name="ID2" direction="in"/>
</symbol>
<symbol name="A31">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16"/>
<pin name="A17"/>
<pin name="A18"/>
<pin name="A19"/>
<pin name="A20"/>
<pin name="A21"/>
<pin name="A22"/>
<pin name="A23"/>
<pin name="A24"/>
<pin name="A25"/>
<pin name="A26"/>
<pin name="A27"/>
<pin name="A28"/>
<pin name="A29"/>
<pin name="A30"/>
<pin name="A31"/>
</symbol>
<symbol name="D47">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D16"/>
<pin name="D17"/>
<pin name="D18"/>
<pin name="D19"/>
<pin name="D20"/>
<pin name="D21"/>
<pin name="D22"/>
<pin name="D23"/>
<pin name="D24"/>
<pin name="D25"/>
<pin name="D26"/>
<pin name="D27"/>
<pin name="D28"/>
<pin name="D29"/>
<pin name="D30"/>
<pin name="D31"/>
<pin name="D32"/>
<pin name="D33"/>
<pin name="D34"/>
<pin name="D35"/>
<pin name="D36"/>
<pin name="D37"/>
<pin name="D38"/>
<pin name="D39"/>
<pin name="D40"/>
<pin name="D41"/>
<pin name="D42"/>
<pin name="D43"/>
<pin name="D44"/>
<pin name="D45"/>
<pin name="D46"/>
<pin name="D47"/>
</symbol>
<symbol name="L0">
<pin name="L0DAT0"/>
<pin name="L0DAT1"/>
<pin name="L0DAT2"/>
<pin name="L0DAT3"/>
<pin name="L0CLK"/>
<pin name="L0ACK"/>
</symbol>
<symbol name="L5">
<pin name="L5DAT0"/>
<pin name="L5DAT1"/>
<pin name="L5DAT2"/>
<pin name="L5DAT3"/>
<pin name="L5CLK"/>
<pin name="L5ACK"/>
</symbol>
<symbol name="L4">
<pin name="L4DAT0"/>
<pin name="L4DAT1"/>
<pin name="L4DAT2"/>
<pin name="L4DAT3"/>
<pin name="L4CLK"/>
<pin name="L4ACK"/>
</symbol>
<symbol name="L3">
<pin name="L3DAT0"/>
<pin name="L3DAT1"/>
<pin name="L3DAT2"/>
<pin name="L3DAT3"/>
<pin name="L3CLK"/>
<pin name="L3ACK"/>
</symbol>
<symbol name="L2">
<pin name="L2DAT0"/>
<pin name="L2DAT1"/>
<pin name="L2DAT2"/>
<pin name="L2DAT3"/>
<pin name="L2CLK"/>
<pin name="L2ACK"/>
</symbol>
<symbol name="L1">
<pin name="L1DAT0"/>
<pin name="L1DAT1"/>
<pin name="L1DAT2"/>
<pin name="L1DAT3"/>
<pin name="L1CLK"/>
<pin name="L1ACK"/>
</symbol>
<symbol name="ADUC812">
<pin name="DAC0" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="CREF" direction="in"/>
<pin name="VREF"/>
<pin name="DGND" direction="pwr"/>
<pin name="DAC1" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SCLOCK" direction="in"/>
<pin name="SDATA/MOSI" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="ADC0/T2" direction="in"/>
<pin name="ADC1/T2EX" direction="in"/>
<pin name="ADC2" direction="in"/>
<pin name="ADC3" direction="in"/>
<pin name="ADC4" direction="in"/>
<pin name="ADC5/!SS" direction="in"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="A8-A16"/>
<pin name="A9-A17"/>
<pin name="A10-A18"/>
<pin name="A11-A19"/>
<pin name="A12-A20"/>
<pin name="A13-A21"/>
<pin name="A14-A22"/>
<pin name="A15-A23"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="P0.0/AD0"/>
<pin name="P0.1/AD1"/>
<pin name="P0.2/AD2"/>
<pin name="P0.3/AD3"/>
<pin name="P0.4/AD4"/>
<pin name="P0.5/AD5"/>
<pin name="P0.6/AD6"/>
<pin name="P0.7/AD7"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="D@GND1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
</symbol>
<symbol name="AD102">
<pin name="FB" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="ICOM" direction="pwr"/>
<pin name="OUT_HI" direction="out"/>
<pin name="OUT_LO" direction="out"/>
<pin name="+15V_DC" direction="out"/>
<pin name="PWRCOM" direction="out"/>
</symbol>
<symbol name="AD104">
<pin name="FB" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="ICOM" direction="pwr"/>
<pin name="OUT_HI" direction="out"/>
<pin name="OUT_LO" direction="out"/>
<pin name="CLK_IN" direction="out"/>
<pin name="PWRCOM" direction="out"/>
</symbol>
<symbol name="AD767">
<pin name="VCC" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="!CS" direction="in"/>
<pin name="SUM_JCT" direction="pas"/>
<pin name="REF_OUT" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="REF_IN" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="B_OFFSET" direction="pas"/>
<pin name="10V" direction="pas"/>
<pin name="20V" direction="pas"/>
<pin name="DGND" direction="pwr"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
</symbol>
<symbol name="AD736">
<pin name="CC" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="CF" direction="pas"/>
<pin name="-VS" direction="pwr"/>
<pin name="CAV" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="COM" direction="pwr"/>
</symbol>
<symbol name="AD536">
<pin name="VIN" direction="in"/>
<pin name="RL" direction="pas"/>
<pin name="-VS" direction="pwr"/>
<pin name="CAV" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="COM" direction="pwr"/>
<pin name="DB" direction="out"/>
<pin name="BIN" direction="in"/>
<pin name="BOUT" direction="out"/>
</symbol>
<symbol name="AD595">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="+C" direction="in"/>
<pin name="-C" direction="in"/>
<pin name="+T" direction="pas"/>
<pin name="-T" direction="pas"/>
<pin name="+ALM" direction="pas"/>
<pin name="-ALM" direction="pas"/>
<pin name="FB" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="VO" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="COM" direction="pwr"/>
</symbol>
<symbol name="AD8801">
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
<pin name="O4" direction="out"/>
<pin name="O5" direction="out"/>
<pin name="O6" direction="out"/>
<pin name="O7" direction="out"/>
<pin name="O8" direction="out"/>
<pin name="!SHDN" direction="in"/>
<pin name="!RS" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!CLK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="VREFH" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AD8803">
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
<pin name="O4" direction="out"/>
<pin name="O5" direction="out"/>
<pin name="O6" direction="out"/>
<pin name="O7" direction="out"/>
<pin name="O8" direction="out"/>
<pin name="!SHDN" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!CLK" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="VREFH" direction="in"/>
<pin name="VREFL" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="OP">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="AD538">
<pin name="IZ" direction="pas"/>
<pin name="VZ" direction="in"/>
<pin name="B" direction="out"/>
<pin name="A" direction="pas"/>
<pin name="IX" direction="pas"/>
<pin name="VX" direction="in"/>
<pin name="IY" direction="pas"/>
<pin name="VY" direction="in"/>
<pin name="C" direction="pas"/>
<pin name="I" direction="pas"/>
<pin name="VO" direction="out"/>
<pin name="D" direction="pas"/>
<pin name="SIGNAL_GND" direction="pwr"/>
<pin name="PWR_GND" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="+10V" direction="out"/>
<pin name="+2V" direction="out"/>
</symbol>
<symbol name="AD654">
<pin name="+VS" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="CT1" direction="pas"/>
<pin name="CT2" direction="pas"/>
<pin name="RT" direction="pas"/>
<pin name="+VIN" direction="in"/>
<pin name="FOUT" direction="oc"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ADSP2189">
<pin name="!RESET" direction="in"/>
<pin name="!BR" direction="in"/>
<pin name="BG" direction="out"/>
<pin name="!BGH" direction="out"/>
<pin name="!DMS" direction="out"/>
<pin name="!PMS" direction="out"/>
<pin name="!IOMS" direction="out"/>
<pin name="!BMS" direction="out"/>
<pin name="!CMS" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="!WR" direction="out"/>
<pin name="MODEA-PF0"/>
<pin name="MODEB-PF1"/>
<pin name="MODEC-PF2"/>
<pin name="MODED-PF3"/>
<pin name="!IRQE!-PF4"/>
<pin name="!IRQL0!-PF5"/>
<pin name="!IRQL1!-PF6"/>
<pin name="!IRQ2!-PF7"/>
<pin name="SCLK1"/>
<pin name="SCLK0"/>
<pin name="!PWD" direction="in"/>
<pin name="!PWDACK" direction="out"/>
<pin name="FL0" direction="out"/>
<pin name="VDDINT" direction="pwr"/>
<pin name="VDDINT@1" direction="pwr"/>
<pin name="VDDEXT" direction="pwr"/>
<pin name="VDDEXT@1" direction="pwr"/>
<pin name="VDDEXT@2" direction="pwr"/>
<pin name="VDDEXT@3" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="!EMS"/>
<pin name="A0" direction="out"/>
<pin name="IAD0-A1" direction="out"/>
<pin name="IAD1-A2" direction="out"/>
<pin name="IAD2-A3" direction="out"/>
<pin name="IAD3-A4" direction="out"/>
<pin name="IAD4-A5" direction="out"/>
<pin name="IAD5-A6" direction="out"/>
<pin name="IAD6-A7" direction="out"/>
<pin name="IAD7-A8" direction="out"/>
<pin name="IAD8-A9" direction="out"/>
<pin name="IAD9-A10" direction="out"/>
<pin name="IAD10-A11" direction="out"/>
<pin name="IAD11-A12" direction="out"/>
<pin name="IAD12-A13" direction="out"/>
<pin name="IAD13-D0"/>
<pin name="IAD14-D1"/>
<pin name="IAD15-D2"/>
<pin name="!IACK!-D3"/>
<pin name="!IS!-D4"/>
<pin name="IAL-D5"/>
<pin name="!IRD!-D6"/>
<pin name="!IWR!-D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D16"/>
<pin name="D17"/>
<pin name="D18"/>
<pin name="D19"/>
<pin name="D20"/>
<pin name="D21"/>
<pin name="D22"/>
<pin name="D23"/>
<pin name="!RFS1!-IRQ0"/>
<pin name="!TFS1!-IRQ1"/>
<pin name="DT1-FO" direction="out"/>
<pin name="DR1-FI" direction="in"/>
<pin name="RFS0"/>
<pin name="TFS0"/>
<pin name="DT0" direction="out"/>
<pin name="DR0" direction="in"/>
<pin name="FL1" direction="out"/>
<pin name="FL2" direction="out"/>
<pin name="!ERESET" direction="in"/>
<pin name="EE" direction="in"/>
<pin name="ECLK" direction="in"/>
<pin name="ECLKOUT" direction="out"/>
<pin name="ELIN" direction="in"/>
<pin name="!EINT" direction="in"/>
<pin name="!EBR" direction="in"/>
<pin name="!EBG" direction="out"/>
<pin name="XTAL" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLKOUT" direction="out"/>
</symbol>
<symbol name="ADSP-21161-ADR">
<pin name="AD0" direction="hiz"/>
<pin name="AD1" direction="hiz"/>
<pin name="AD2" direction="hiz"/>
<pin name="AD3" direction="hiz"/>
<pin name="AD4" direction="hiz"/>
<pin name="AD5" direction="hiz"/>
<pin name="AD6" direction="hiz"/>
<pin name="AD7" direction="hiz"/>
<pin name="AD8" direction="hiz"/>
<pin name="AD9" direction="hiz"/>
<pin name="AD10" direction="hiz"/>
<pin name="AD11" direction="hiz"/>
<pin name="AD12" direction="hiz"/>
<pin name="AD13" direction="hiz"/>
<pin name="AD14" direction="hiz"/>
<pin name="AD15" direction="hiz"/>
<pin name="AD16" direction="hiz"/>
<pin name="AD17" direction="hiz"/>
<pin name="AD18" direction="hiz"/>
<pin name="AD19" direction="hiz"/>
<pin name="AD20" direction="hiz"/>
<pin name="AD21" direction="hiz"/>
<pin name="AD22" direction="hiz"/>
<pin name="AD23" direction="hiz"/>
</symbol>
<symbol name="ADSP-21161-DATA">
<pin name="D16" direction="hiz"/>
<pin name="D17" direction="hiz"/>
<pin name="D18" direction="hiz"/>
<pin name="D19" direction="hiz"/>
<pin name="D20" direction="hiz"/>
<pin name="D21" direction="hiz"/>
<pin name="D22" direction="hiz"/>
<pin name="D23" direction="hiz"/>
<pin name="D24" direction="hiz"/>
<pin name="D25" direction="hiz"/>
<pin name="D26" direction="hiz"/>
<pin name="D27" direction="hiz"/>
<pin name="D28" direction="hiz"/>
<pin name="D29" direction="hiz"/>
<pin name="D30" direction="hiz"/>
<pin name="D31" direction="hiz"/>
<pin name="D32" direction="hiz"/>
<pin name="D33" direction="hiz"/>
<pin name="D34" direction="hiz"/>
<pin name="D35" direction="hiz"/>
<pin name="D36" direction="hiz"/>
<pin name="D37" direction="hiz"/>
<pin name="D38" direction="hiz"/>
<pin name="D39" direction="hiz"/>
<pin name="D40" direction="hiz"/>
<pin name="D41" direction="hiz"/>
<pin name="D42" direction="hiz"/>
<pin name="D43" direction="hiz"/>
<pin name="D44" direction="hiz"/>
<pin name="D45" direction="hiz"/>
<pin name="D46" direction="hiz"/>
<pin name="D47" direction="hiz"/>
</symbol>
<symbol name="ADSP-21161-CTRL1">
<pin name="!IRQ0" direction="in"/>
<pin name="!IRQ1" direction="in"/>
<pin name="!IRQ2" direction="in"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="FLAG4"/>
<pin name="FLAG5"/>
<pin name="FLAG6"/>
<pin name="FLAG7"/>
<pin name="FLAG8"/>
<pin name="FLAG9"/>
<pin name="FLAG10"/>
<pin name="FLAG11"/>
<pin name="TIMEXP" direction="out"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="ID2" direction="in"/>
<pin name="RPBA" direction="in"/>
<pin name="EBOOT" direction="in"/>
<pin name="LBOOT" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="XTAL" direction="out"/>
<pin name="CLK_CFG0" direction="in"/>
<pin name="CLK_CFG1" direction="in"/>
<pin name="!CLKDBL" direction="in"/>
</symbol>
<symbol name="ADSP-21161-CTRL2">
<pin name="!MS0" direction="hiz"/>
<pin name="!MS1" direction="hiz"/>
<pin name="!MS2" direction="hiz"/>
<pin name="!RD" direction="hiz"/>
<pin name="!WR" direction="hiz"/>
<pin name="BRST" direction="hiz"/>
<pin name="ACK"/>
<pin name="!SBTS" direction="in"/>
<pin name="!CAS"/>
<pin name="!RAS"/>
<pin name="!SDWE"/>
<pin name="DQM" direction="out"/>
<pin name="SDCLK0"/>
<pin name="SDCLK1" direction="out"/>
<pin name="SDCKE"/>
<pin name="SDA10" direction="out"/>
<pin name="!HBR" direction="in"/>
<pin name="!HBG"/>
<pin name="!CS" direction="in"/>
<pin name="REDY" direction="out"/>
<pin name="!DMAR1" direction="in"/>
<pin name="!DMAR2" direction="in"/>
<pin name="!DMAG1" direction="out"/>
<pin name="!DMAG2" direction="out"/>
<pin name="!BR1"/>
<pin name="!BR2"/>
<pin name="!BR3"/>
<pin name="!BR4"/>
<pin name="!BR5"/>
<pin name="!BR6"/>
<pin name="BMSTR" direction="out"/>
<pin name="!PA"/>
<pin name="!BMS"/>
<pin name="CLKOUT" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="!MS3" direction="hiz"/>
<pin name="!TRST" direction="in"/>
<pin name="!EMU" direction="out"/>
</symbol>
<symbol name="ADSP-21161-SER">
<pin name="D0A"/>
<pin name="D0B"/>
<pin name="SCLK0"/>
<pin name="FS0"/>
<pin name="SPICLK"/>
<pin name="!SPIDS" direction="in"/>
<pin name="MOSI"/>
<pin name="MISO"/>
<pin name="D1A"/>
<pin name="D1B"/>
<pin name="SCLK1"/>
<pin name="FS1"/>
<pin name="D2A"/>
<pin name="D2B"/>
<pin name="SCLK2"/>
<pin name="FS2"/>
<pin name="D3A"/>
<pin name="D3B"/>
<pin name="SCLK3"/>
<pin name="FS3"/>
</symbol>
<symbol name="ADSP-21161-PAR">
<pin name="L0CLK"/>
<pin name="L0ACK"/>
<pin name="L0DAT0"/>
<pin name="L0DAT1"/>
<pin name="L0DAT2"/>
<pin name="L0DAT3"/>
<pin name="L0DAT4"/>
<pin name="L0DAT5"/>
<pin name="L0DAT6"/>
<pin name="L0DAT7"/>
<pin name="L1CLK"/>
<pin name="L1ACK"/>
<pin name="L1DAT0"/>
<pin name="L1DAT1"/>
<pin name="L1DAT2"/>
<pin name="L1DAT3"/>
<pin name="L1DAT4"/>
<pin name="L1DAT5"/>
<pin name="L1DAT6"/>
<pin name="L1DAT7"/>
</symbol>
<symbol name="VDDEXT">
<pin name="VDDEXT" direction="pwr"/>
</symbol>
<symbol name="VDDINT">
<pin name="VDDINT" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AVDD">
<pin name="AVDD" direction="pwr"/>
</symbol>
<symbol name="AGND">
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="ADUC814">
<pin name="DGND" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="DLOAD" direction="in"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/!CONVST"/>
<pin name="P1.0/T2"/>
<pin name="P1.1/T2EX"/>
<pin name="P1.2/ADC0"/>
<pin name="P1.3/ADC1"/>
<pin name="P1.4/ADC2"/>
<pin name="P1.5/ADC3"/>
<pin name="P1.6/ADC4/DAC0"/>
<pin name="P1.7/ADC5/DAC1"/>
<pin name="P3.5/T1/!SS!/EXTCLK"/>
<pin name="P3.6/MISO"/>
<pin name="P3.7/MOSI"/>
<pin name="SCLOCK"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="CREF" direction="pas"/>
<pin name="VREF" direction="pas"/>
</symbol>
<symbol name="ADXL202">
<pin name="ST" direction="in"/>
<pin name="T2" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="YOUT" direction="in"/>
<pin name="XOUT" direction="in"/>
<pin name="YFILT" direction="in"/>
<pin name="XFILT" direction="in"/>
<pin name="VDD" direction="in"/>
</symbol>
<symbol name="AD650">
<pin name="VOUT" direction="out"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="BOC" direction="pas"/>
<pin name="-VS" direction="in"/>
<pin name="ONESHOT" direction="pas"/>
<pin name="FOUT" direction="out"/>
<pin name="COMP_IN" direction="in"/>
<pin name="DGND" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="+VS" direction="in"/>
<pin name="OFF0" direction="in"/>
<pin name="OFF1" direction="in"/>
</symbol>
<symbol name="AD7524">
<pin name="VREF" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="!CS" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="RFB" direction="pas"/>
<pin name="OUT1" direction="pas"/>
<pin name="OUT2" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AD7568">
<pin name="VDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="!FSIN" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="SDIN" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="SDOUT" direction="in"/>
<pin name="!LDAG" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="RFBA" direction="pas"/>
<pin name="RFBB" direction="pas"/>
<pin name="RFBC" direction="pas"/>
<pin name="RFBD" direction="pas"/>
<pin name="RFBE" direction="pas"/>
<pin name="RFBF" direction="pas"/>
<pin name="RFBG" direction="pas"/>
<pin name="RFBH" direction="pas"/>
<pin name="VREFA" direction="pas"/>
<pin name="VREFB" direction="pas"/>
<pin name="VREFC" direction="pas"/>
<pin name="VREFD" direction="pas"/>
<pin name="VREFE" direction="pas"/>
<pin name="VREFF" direction="pas"/>
<pin name="VREFG" direction="pas"/>
<pin name="VREFH" direction="pas"/>
<pin name="IOUT1A" direction="pas"/>
<pin name="IOUT2A" direction="pas"/>
<pin name="IOUT1B" direction="pas"/>
<pin name="IOUT2B" direction="pas"/>
<pin name="IOUT1C" direction="pas"/>
<pin name="IOUT2C" direction="pas"/>
<pin name="IOUT1D" direction="pas"/>
<pin name="IOUT2D" direction="pas"/>
<pin name="IOUT1E" direction="pas"/>
<pin name="IOUT2E" direction="pas"/>
<pin name="IOUT1F" direction="pas"/>
<pin name="IOUT2F" direction="pas"/>
<pin name="IOUT1G" direction="pas"/>
<pin name="IOUT2G" direction="pas"/>
<pin name="IOUT1H" direction="pas"/>
<pin name="IOUT2H" direction="pas"/>
</symbol>
<symbol name="ADSP_BF533_MBGA">
<pin name="ADDR1" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="AMS_B0" direction="out"/>
<pin name="AMS_B1" direction="out"/>
<pin name="AMS_B2" direction="out"/>
<pin name="AMS_B3" direction="out"/>
<pin name="AOE_B" direction="out"/>
<pin name="ARDY" direction="in"/>
<pin name="ARE_B" direction="out"/>
<pin name="AWE_B" direction="out"/>
<pin name="ABE_B0" direction="out"/>
<pin name="ABE_B1" direction="out"/>
<pin name="BG_B" direction="hiz"/>
<pin name="BGH_B" direction="hiz"/>
<pin name="BMODE0" direction="in"/>
<pin name="BMODE1" direction="in"/>
<pin name="BR_B" direction="in"/>
<pin name="DR0PRI" direction="in"/>
<pin name="DR0SEC" direction="in"/>
<pin name="DR1PRI" direction="in"/>
<pin name="DR1SEC" direction="in"/>
<pin name="DT0PRI" direction="out"/>
<pin name="DT0SEC" direction="out"/>
<pin name="DT1PRI" direction="out"/>
<pin name="DT1SEC" direction="out"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="NMI" direction="in"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PP_CLK" direction="in"/>
<pin name="PP0"/>
<pin name="PP1"/>
<pin name="PP2"/>
<pin name="PP3"/>
<pin name="RESET_B" direction="in"/>
<pin name="RFS0"/>
<pin name="RFS1"/>
<pin name="RSCLK0"/>
<pin name="RSCLK1"/>
<pin name="TSCLK0"/>
<pin name="TSCLK1"/>
<pin name="CLKOUT" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="hiz"/>
<pin name="SA10" direction="out"/>
<pin name="SCAS_B" direction="out"/>
<pin name="SCK"/>
<pin name="SCKE" direction="out"/>
<pin name="SMS_B" direction="out"/>
<pin name="SRAS_B" direction="out"/>
<pin name="SWE_B" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRST_B" direction="in"/>
<pin name="EMU_B" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="TFS0"/>
<pin name="TFS1"/>
<pin name="TMR0"/>
<pin name="TMR1"/>
<pin name="TMR2"/>
<pin name="RTXI" direction="pwr"/>
<pin name="RTXO" direction="pwr"/>
<pin name="VDD_INT@0" direction="pwr"/>
<pin name="VDD_INT@1" direction="pwr"/>
<pin name="VDD_INT@2" direction="pwr"/>
<pin name="VDD_INT@3" direction="pwr"/>
<pin name="VDD_INT@4" direction="pwr"/>
<pin name="VDD_INT@5" direction="pwr"/>
<pin name="VDD_EXT@0" direction="pwr"/>
<pin name="VDD_EXT@1" direction="pwr"/>
<pin name="VDD_EXT@2" direction="pwr"/>
<pin name="VDD_EXT@3" direction="pwr"/>
<pin name="VDD_EXT@4" direction="pwr"/>
<pin name="VDD_EXT@5" direction="pwr"/>
<pin name="VDD_EXT@6" direction="pwr"/>
<pin name="VDD_EXT@7" direction="pwr"/>
<pin name="VDD_EXT@8" direction="pwr"/>
<pin name="VDD_EXT@9" direction="pwr"/>
<pin name="VDD_EXT@10" direction="pwr"/>
<pin name="VDD_EXT@11" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="VDD_RTC" direction="pwr"/>
<pin name="CLKIN" direction="pwr"/>
<pin name="XTAL" direction="pwr"/>
<pin name="VROUT@0" direction="pwr"/>
<pin name="VROUT@1" direction="pwr"/>
</symbol>
<symbol name="AD8133">
<pin name="VS-@1" direction="pwr"/>
<pin name="VS-@2" direction="pwr"/>
<pin name="VS-@3" direction="pwr"/>
<pin name="VS-@4" direction="pwr"/>
<pin name="VS+@1" direction="pwr"/>
<pin name="VS+@2" direction="pwr"/>
<pin name="VS+@3" direction="pwr"/>
<pin name="VS+@4" direction="pwr"/>
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+OUTA" direction="out"/>
<pin name="-OUTA" direction="out"/>
<pin name="VCOMA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+OUTB" direction="out"/>
<pin name="-OUTB" direction="out"/>
<pin name="VCOMB" direction="in"/>
<pin name="+INC" direction="in"/>
<pin name="-INC" direction="in"/>
<pin name="+OUTC" direction="out"/>
<pin name="-OUTC" direction="out"/>
<pin name="VCOMC" direction="in"/>
<pin name="OPD" direction="in"/>
</symbol>
<symbol name="33170285923617ADSP_BF531_MBGA">
<pin name="ADDR1" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="AMS_B0" direction="out"/>
<pin name="AMS_B1" direction="out"/>
<pin name="AMS_B2" direction="out"/>
<pin name="AMS_B3" direction="out"/>
<pin name="AOE_B" direction="out"/>
<pin name="ARDY" direction="in"/>
<pin name="ARE_B" direction="out"/>
<pin name="AWE_B" direction="out"/>
<pin name="ABE_B0" direction="out"/>
<pin name="ABE_B1" direction="out"/>
<pin name="BG_B" direction="hiz"/>
<pin name="BGH_B" direction="hiz"/>
<pin name="BMODE0" direction="in"/>
<pin name="BMODE1" direction="in"/>
<pin name="BR_B" direction="in"/>
<pin name="DR0PRI" direction="in"/>
<pin name="DR0SEC" direction="in"/>
<pin name="DR1PRI" direction="in"/>
<pin name="DR1SEC" direction="in"/>
<pin name="DT0PRI" direction="out"/>
<pin name="DT0SEC" direction="out"/>
<pin name="DT1PRI" direction="out"/>
<pin name="DT1SEC" direction="out"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="NMI" direction="in"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PP_CLK" direction="in"/>
<pin name="PP0"/>
<pin name="PP1"/>
<pin name="PP2"/>
<pin name="PP3"/>
<pin name="RESET_B" direction="in"/>
<pin name="RFS0"/>
<pin name="RFS1"/>
<pin name="RSCLK0"/>
<pin name="RSCLK1"/>
<pin name="TSCLK0"/>
<pin name="TSCLK1"/>
<pin name="CLKOUT" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="hiz"/>
<pin name="SA10" direction="out"/>
<pin name="SCAS_B" direction="out"/>
<pin name="SCK"/>
<pin name="SCKE" direction="out"/>
<pin name="SMS_B" direction="out"/>
<pin name="SRAS_B" direction="out"/>
<pin name="SWE_B" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRST_B" direction="in"/>
<pin name="EMU_B" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="TFS0"/>
<pin name="TFS1"/>
<pin name="TMR0"/>
<pin name="TMR1"/>
<pin name="TMR2"/>
<pin name="RTXI" direction="pwr"/>
<pin name="RTXO" direction="pwr"/>
<pin name="VDD_INT@0" direction="pwr"/>
<pin name="VDD_INT@1" direction="pwr"/>
<pin name="VDD_INT@2" direction="pwr"/>
<pin name="VDD_INT@3" direction="pwr"/>
<pin name="VDD_INT@4" direction="pwr"/>
<pin name="VDD_INT@5" direction="pwr"/>
<pin name="VDD_EXT@0" direction="pwr"/>
<pin name="VDD_EXT@1" direction="pwr"/>
<pin name="VDD_EXT@2" direction="pwr"/>
<pin name="VDD_EXT@3" direction="pwr"/>
<pin name="VDD_EXT@4" direction="pwr"/>
<pin name="VDD_EXT@5" direction="pwr"/>
<pin name="VDD_EXT@6" direction="pwr"/>
<pin name="VDD_EXT@7" direction="pwr"/>
<pin name="VDD_EXT@8" direction="pwr"/>
<pin name="VDD_EXT@9" direction="pwr"/>
<pin name="VDD_EXT@10" direction="pwr"/>
<pin name="VDD_EXT@11" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="VDD_RTC" direction="pwr"/>
<pin name="CLKIN" direction="pwr"/>
<pin name="XTAL" direction="pwr"/>
<pin name="VROUT@0" direction="pwr"/>
<pin name="VROUT@1" direction="pwr"/>
</symbol>
<symbol name="33335272594765ADSP_BF532_MBGA">
<pin name="ADDR1" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="AMS_B0" direction="out"/>
<pin name="AMS_B1" direction="out"/>
<pin name="AMS_B2" direction="out"/>
<pin name="AMS_B3" direction="out"/>
<pin name="AOE_B" direction="out"/>
<pin name="ARDY" direction="in"/>
<pin name="ARE_B" direction="out"/>
<pin name="AWE_B" direction="out"/>
<pin name="ABE_B0" direction="out"/>
<pin name="ABE_B1" direction="out"/>
<pin name="BG_B" direction="hiz"/>
<pin name="BGH_B" direction="hiz"/>
<pin name="BMODE0" direction="in"/>
<pin name="BMODE1" direction="in"/>
<pin name="BR_B" direction="in"/>
<pin name="DR0PRI" direction="in"/>
<pin name="DR0SEC" direction="in"/>
<pin name="DR1PRI" direction="in"/>
<pin name="DR1SEC" direction="in"/>
<pin name="DT0PRI" direction="out"/>
<pin name="DT0SEC" direction="out"/>
<pin name="DT1PRI" direction="out"/>
<pin name="DT1SEC" direction="out"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="NMI" direction="in"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PP_CLK" direction="in"/>
<pin name="PP0"/>
<pin name="PP1"/>
<pin name="PP2"/>
<pin name="PP3"/>
<pin name="RESET_B" direction="in"/>
<pin name="RFS0"/>
<pin name="RFS1"/>
<pin name="RSCLK0"/>
<pin name="RSCLK1"/>
<pin name="TSCLK0"/>
<pin name="TSCLK1"/>
<pin name="CLKOUT" direction="out"/>
<pin name="RX" direction="in"/>
<pin name="TX" direction="hiz"/>
<pin name="SA10" direction="out"/>
<pin name="SCAS_B" direction="out"/>
<pin name="SCK"/>
<pin name="SCKE" direction="out"/>
<pin name="SMS_B" direction="out"/>
<pin name="SRAS_B" direction="out"/>
<pin name="SWE_B" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRST_B" direction="in"/>
<pin name="EMU_B" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="TFS0"/>
<pin name="TFS1"/>
<pin name="TMR0"/>
<pin name="TMR1"/>
<pin name="TMR2"/>
<pin name="RTXI" direction="pwr"/>
<pin name="RTXO" direction="pwr"/>
<pin name="VDD_INT@0" direction="pwr"/>
<pin name="VDD_INT@1" direction="pwr"/>
<pin name="VDD_INT@2" direction="pwr"/>
<pin name="VDD_INT@3" direction="pwr"/>
<pin name="VDD_INT@4" direction="pwr"/>
<pin name="VDD_INT@5" direction="pwr"/>
<pin name="VDD_EXT@0" direction="pwr"/>
<pin name="VDD_EXT@1" direction="pwr"/>
<pin name="VDD_EXT@2" direction="pwr"/>
<pin name="VDD_EXT@3" direction="pwr"/>
<pin name="VDD_EXT@4" direction="pwr"/>
<pin name="VDD_EXT@5" direction="pwr"/>
<pin name="VDD_EXT@6" direction="pwr"/>
<pin name="VDD_EXT@7" direction="pwr"/>
<pin name="VDD_EXT@8" direction="pwr"/>
<pin name="VDD_EXT@9" direction="pwr"/>
<pin name="VDD_EXT@10" direction="pwr"/>
<pin name="VDD_EXT@11" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="VDD_RTC" direction="pwr"/>
<pin name="CLKIN" direction="pwr"/>
<pin name="XTAL" direction="pwr"/>
<pin name="VROUT@0" direction="pwr"/>
<pin name="VROUT@1" direction="pwr"/>
</symbol>
<symbol name="ADSP-BF537">
<pin name="ADDR1" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="AMS_B0" direction="out"/>
<pin name="AMS_B1" direction="out"/>
<pin name="AMS_B2" direction="out"/>
<pin name="AMS_B3" direction="out"/>
<pin name="AOE_B" direction="out"/>
<pin name="ARDY" direction="in"/>
<pin name="ARE_B" direction="out"/>
<pin name="AWE_B" direction="out"/>
<pin name="ABE_B0" direction="out"/>
<pin name="ABE_B1" direction="out"/>
<pin name="BG_B" direction="hiz"/>
<pin name="BGH_B" direction="hiz"/>
<pin name="BMODE0" direction="in"/>
<pin name="BMODE1" direction="in"/>
<pin name="BMODE2" direction="in"/>
<pin name="BR_B" direction="in"/>
<pin name="DR0PRI"/>
<pin name="DR0SEC"/>
<pin name="DT0PRI"/>
<pin name="DT0SEC"/>
<pin name="NMI" direction="in"/>
<pin name="MDC"/>
<pin name="MDIO"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PF16"/>
<pin name="PF17"/>
<pin name="PF18"/>
<pin name="PF19"/>
<pin name="PF20"/>
<pin name="PF21"/>
<pin name="PF22"/>
<pin name="PF23"/>
<pin name="PF24"/>
<pin name="PF25"/>
<pin name="PF26"/>
<pin name="PF27"/>
<pin name="PF28"/>
<pin name="PF29"/>
<pin name="PF30"/>
<pin name="PF31"/>
<pin name="PF32"/>
<pin name="PF33"/>
<pin name="PF34"/>
<pin name="PF35"/>
<pin name="PF36"/>
<pin name="PF37"/>
<pin name="PF38"/>
<pin name="PF39"/>
<pin name="PF40"/>
<pin name="PF41"/>
<pin name="PF42"/>
<pin name="PF43"/>
<pin name="PF44"/>
<pin name="PF45"/>
<pin name="PF46"/>
<pin name="PF47"/>
<pin name="RESET_B" direction="in"/>
<pin name="RFS0"/>
<pin name="RSCLK0"/>
<pin name="TSCLK0"/>
<pin name="CLKOUT" direction="out"/>
<pin name="SA10" direction="out"/>
<pin name="SCAS_B" direction="out"/>
<pin name="SCKE" direction="out"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="SMS_B" direction="out"/>
<pin name="SRAS_B" direction="out"/>
<pin name="SWE_B" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRST_B" direction="in"/>
<pin name="EMU_B" direction="pwr"/>
<pin name="TFS0"/>
<pin name="RTXI" direction="pwr"/>
<pin name="RTXO" direction="pwr"/>
<pin name="TEST" direction="in"/>
<pin name="VDD_INT@0" direction="pwr"/>
<pin name="VDD_INT@1" direction="pwr"/>
<pin name="VDD_INT@2" direction="pwr"/>
<pin name="VDD_INT@3" direction="pwr"/>
<pin name="VDD_INT@4" direction="pwr"/>
<pin name="VDD_INT@5" direction="pwr"/>
<pin name="VDD_INT@6" direction="pwr"/>
<pin name="VDD_INT@7" direction="pwr"/>
<pin name="VDD_INT@8" direction="pwr"/>
<pin name="VDD_INT@9" direction="pwr"/>
<pin name="VDD_INT@10" direction="pwr"/>
<pin name="VDD_INT@11" direction="pwr"/>
<pin name="VDD_EXT@0" direction="pwr"/>
<pin name="VDD_EXT@1" direction="pwr"/>
<pin name="VDD_EXT@2" direction="pwr"/>
<pin name="VDD_EXT@3" direction="pwr"/>
<pin name="VDD_EXT@4" direction="pwr"/>
<pin name="VDD_EXT@5" direction="pwr"/>
<pin name="VDD_EXT@6" direction="pwr"/>
<pin name="VDD_EXT@7" direction="pwr"/>
<pin name="VDD_EXT@8" direction="pwr"/>
<pin name="VDD_EXT@9" direction="pwr"/>
<pin name="VDD_EXT@10" direction="pwr"/>
<pin name="VDD_EXT@11" direction="pwr"/>
<pin name="VDD_EXT@12" direction="pwr"/>
<pin name="VDD_EXT@13" direction="pwr"/>
<pin name="VDD_EXT@14" direction="pwr"/>
<pin name="VDD_EXT@15" direction="pwr"/>
<pin name="VDD_EXT@16" direction="pwr"/>
<pin name="VDD_EXT@17" direction="pwr"/>
<pin name="VDD_EXT@18" direction="pwr"/>
<pin name="VDD_EXT@19" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="VDD_RTC" direction="pwr"/>
<pin name="CLKIN" direction="pwr"/>
<pin name="XTAL" direction="pwr"/>
<pin name="BUF_XTAL" direction="pwr"/>
<pin name="VROUT@0" direction="pwr"/>
<pin name="VROUT@1" direction="pwr"/>
</symbol>
<symbol name="ADSP_21535">
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="ADDR20" direction="out"/>
<pin name="ADDR21" direction="out"/>
<pin name="ADDR22" direction="out"/>
<pin name="ADDR23" direction="out"/>
<pin name="ADDR24" direction="out"/>
<pin name="ADDR25" direction="out"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="DATA16"/>
<pin name="DATA17"/>
<pin name="DATA18"/>
<pin name="DATA19"/>
<pin name="DATA20"/>
<pin name="DATA21"/>
<pin name="DATA22"/>
<pin name="DATA23"/>
<pin name="DATA24"/>
<pin name="DATA25"/>
<pin name="DATA26"/>
<pin name="DATA27"/>
<pin name="DATA28"/>
<pin name="DATA29"/>
<pin name="DATA30"/>
<pin name="DATA31"/>
<pin name="EMU_B" direction="out"/>
<pin name="BYPASS" direction="in"/>
<pin name="SLEEP" direction="out"/>
<pin name="BMODE0" direction="in"/>
<pin name="BMODE1" direction="in"/>
<pin name="BMODE2" direction="in"/>
<pin name="PCI_INTD" direction="in"/>
<pin name="PCI_INTC" direction="in"/>
<pin name="PCI_INTB" direction="in"/>
<pin name="PCI_INTA"/>
<pin name="PCI_CLK" direction="in"/>
<pin name="PCI_LOCK" direction="in"/>
<pin name="PCI_SERR"/>
<pin name="PCI_PAR"/>
<pin name="PCI_PERR"/>
<pin name="PCI_STOP"/>
<pin name="PCI_DEVSEL"/>
<pin name="PCI_TRDY"/>
<pin name="PCI_FRAME"/>
<pin name="PCI_IDSEL" direction="in"/>
<pin name="PCI_GNT" direction="in"/>
<pin name="PCI_REQ" direction="out"/>
<pin name="PCI_RST"/>
<pin name="PCI_IRDY"/>
<pin name="PCI_CBE0"/>
<pin name="PCI_CBE1"/>
<pin name="PCI_CBE2"/>
<pin name="PCI_CBE3"/>
<pin name="PCI_AD0"/>
<pin name="PCI_AD1"/>
<pin name="PCI_AD2"/>
<pin name="PCI_AD3"/>
<pin name="PCI_AD4"/>
<pin name="PCI_AD5"/>
<pin name="PCI_AD6"/>
<pin name="PCI_AD7"/>
<pin name="PCI_AD8"/>
<pin name="PCI_AD9"/>
<pin name="PCI_AD10"/>
<pin name="PCI_AD11"/>
<pin name="PCI_AD12"/>
<pin name="PCI_AD13"/>
<pin name="PCI_AD14"/>
<pin name="PCI_AD15"/>
<pin name="PCI_AD16"/>
<pin name="PCI_AD17"/>
<pin name="PCI_AD18"/>
<pin name="PCI_AD19"/>
<pin name="PCI_AD20"/>
<pin name="PCI_AD21"/>
<pin name="PCI_AD22"/>
<pin name="PCI_AD23"/>
<pin name="PCI_AD24"/>
<pin name="PCI_AD25"/>
<pin name="PCI_AD26"/>
<pin name="PCI_AD27"/>
<pin name="PCI_AD28"/>
<pin name="PCI_AD29"/>
<pin name="PCI_AD30"/>
<pin name="PCI_AD31"/>
<pin name="SCK1"/>
<pin name="MISO1"/>
<pin name="MOSI1"/>
<pin name="SCK0"/>
<pin name="MISO0"/>
<pin name="MOSI0"/>
<pin name="DT1" direction="out"/>
<pin name="TFS1"/>
<pin name="TSCLK1"/>
<pin name="DR1" direction="in"/>
<pin name="RFS1"/>
<pin name="RSCLK1"/>
<pin name="DT0" direction="out"/>
<pin name="TFS0"/>
<pin name="TSCLK0"/>
<pin name="DR0" direction="in"/>
<pin name="RFS0"/>
<pin name="RSCLK0"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="ARDY" direction="in"/>
<pin name="SCAS_B" direction="out"/>
<pin name="SMS_B0" direction="out"/>
<pin name="SMS_B1" direction="out"/>
<pin name="SMS_B2" direction="out"/>
<pin name="SMS_B3" direction="out"/>
<pin name="SWE_B" direction="out"/>
<pin name="SRAS_B" direction="out"/>
<pin name="SA10" direction="out"/>
<pin name="SCKE" direction="out"/>
<pin name="SCLK0" direction="hiz"/>
<pin name="CLKOUT_SCLK1" direction="hiz"/>
<pin name="AWE_B" direction="out"/>
<pin name="ARE_B" direction="out"/>
<pin name="AOE_B" direction="out"/>
<pin name="AMS_B0" direction="out"/>
<pin name="AMS_B1" direction="out"/>
<pin name="AMS_B2" direction="out"/>
<pin name="AMS_B3" direction="out"/>
<pin name="ABE_B_SDQM0" direction="out"/>
<pin name="ABE_B_SDQM1" direction="out"/>
<pin name="ABE_B_SDQM2" direction="out"/>
<pin name="ABE_B_SDQM3" direction="out"/>
<pin name="TMR0"/>
<pin name="TMR1"/>
<pin name="TMR2"/>
<pin name="RX0" direction="in"/>
<pin name="TX0" direction="out"/>
<pin name="RX1" direction="in"/>
<pin name="TX1" direction="out"/>
<pin name="USB_CLK" direction="in"/>
<pin name="XVER_DATA" direction="in"/>
<pin name="RESET_B" direction="in"/>
<pin name="DPLS" direction="in"/>
<pin name="DMNS" direction="in"/>
<pin name="TXDPLS" direction="out"/>
<pin name="TXDMNS" direction="out"/>
<pin name="TXEN" direction="out"/>
<pin name="SUSPEND" direction="out"/>
<pin name="NMI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST_B" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="CLKIN1" direction="pwr"/>
<pin name="XTALI" direction="pwr"/>
<pin name="XTALO" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="NC@0" direction="pwr"/>
<pin name="NC@1" direction="pwr"/>
<pin name="NC@2" direction="pwr"/>
<pin name="NC@3" direction="pwr"/>
<pin name="VDDEXT@0" direction="pwr"/>
<pin name="VDDEXT@1" direction="pwr"/>
<pin name="VDDEXT@2" direction="pwr"/>
<pin name="VDDEXT@3" direction="pwr"/>
<pin name="VDDEXT@4" direction="pwr"/>
<pin name="VDDEXT@5" direction="pwr"/>
<pin name="VDDEXT@6" direction="pwr"/>
<pin name="VDDEXT@7" direction="pwr"/>
<pin name="VDDEXT@8" direction="pwr"/>
<pin name="VDDEXT@9" direction="pwr"/>
<pin name="VDDINT@0" direction="pwr"/>
<pin name="VDDINT@1" direction="pwr"/>
<pin name="VDDINT@2" direction="pwr"/>
<pin name="VDDINT@3" direction="pwr"/>
<pin name="VDDINT@4" direction="pwr"/>
<pin name="VDDINT@5" direction="pwr"/>
<pin name="VDDINT@6" direction="pwr"/>
<pin name="VDDINT@7" direction="pwr"/>
<pin name="VDDINT@8" direction="pwr"/>
<pin name="VDDINT@9" direction="pwr"/>
<pin name="VDDINT@10" direction="pwr"/>
<pin name="VDDINT@11" direction="pwr"/>
<pin name="VDDINT@12" direction="pwr"/>
<pin name="VDDPCIEXT@0" direction="pwr"/>
<pin name="VDDPCIEXT@1" direction="pwr"/>
<pin name="VDDPCIEXT@2" direction="pwr"/>
<pin name="VDDPCIEXT@3" direction="pwr"/>
<pin name="VDDPCIEXT@4" direction="pwr"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="VDDRTC" direction="pwr"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="VSSRTC" direction="pwr"/>
</symbol>
<symbol name="AD6624A">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="CHIP_ID0" direction="in"/>
<pin name="CHIP_ID1" direction="in"/>
<pin name="CHIP_ID2" direction="in"/>
<pin name="CHIP_ID3" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="EXPA0" direction="in"/>
<pin name="EXPA1" direction="in"/>
<pin name="EXPA2" direction="in"/>
<pin name="EXPB0" direction="in"/>
<pin name="EXPB1" direction="in"/>
<pin name="EXPB2" direction="in"/>
<pin name="IENA" direction="in"/>
<pin name="IENB" direction="in"/>
<pin name="INA0" direction="in"/>
<pin name="INA1" direction="in"/>
<pin name="INA10" direction="in"/>
<pin name="INA11" direction="in"/>
<pin name="INA12" direction="in"/>
<pin name="INA13" direction="in"/>
<pin name="INA2" direction="in"/>
<pin name="INA3" direction="in"/>
<pin name="INA4" direction="in"/>
<pin name="INA5" direction="in"/>
<pin name="INA6" direction="in"/>
<pin name="INA7" direction="in"/>
<pin name="INA8" direction="in"/>
<pin name="INA9" direction="in"/>
<pin name="INB0" direction="in"/>
<pin name="INB1" direction="in"/>
<pin name="INB10" direction="in"/>
<pin name="INB11" direction="in"/>
<pin name="INB12" direction="in"/>
<pin name="INB13" direction="in"/>
<pin name="INB2" direction="in"/>
<pin name="INB3" direction="in"/>
<pin name="INB4" direction="in"/>
<pin name="INB5" direction="in"/>
<pin name="INB6" direction="in"/>
<pin name="INB7" direction="in"/>
<pin name="INB8" direction="in"/>
<pin name="INB9" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="R_W" direction="in"/>
<pin name="SBM0" direction="in"/>
<pin name="SDIN0" direction="in"/>
<pin name="SDIN1" direction="in"/>
<pin name="SDIN2" direction="in"/>
<pin name="SDIN3" direction="in"/>
<pin name="SDIV0" direction="in"/>
<pin name="SDIV1" direction="in"/>
<pin name="SDIV2" direction="in"/>
<pin name="SDIV3" direction="in"/>
<pin name="SYNCA" direction="in"/>
<pin name="SYNCB" direction="in"/>
<pin name="SYNCC" direction="in"/>
<pin name="SYNCD" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="DS" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="SCLK0"/>
<pin name="SCLK1"/>
<pin name="SCLK2"/>
<pin name="SCLK3"/>
<pin name="SDFS0"/>
<pin name="SDFS1"/>
<pin name="SDFS2"/>
<pin name="SDFS3"/>
<pin name="SDO0" direction="out"/>
<pin name="SDO1" direction="out"/>
<pin name="SDO2" direction="out"/>
<pin name="SDO3" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="DTACK" direction="out"/>
<pin name="LIA_A" direction="hiz"/>
<pin name="LIA_B" direction="hiz"/>
<pin name="LIB_A" direction="hiz"/>
<pin name="LIB_B" direction="hiz"/>
<pin name="SDFE0" direction="hiz"/>
<pin name="SDFE1" direction="hiz"/>
<pin name="SDFE2" direction="hiz"/>
<pin name="SDFE3" direction="hiz"/>
<pin name="DR0" direction="hiz"/>
<pin name="DR1" direction="hiz"/>
<pin name="DR2" direction="hiz"/>
<pin name="DR3" direction="hiz"/>
<pin name="VDDCORE@1" direction="pwr"/>
<pin name="VDDCORE@2" direction="pwr"/>
<pin name="VDDCORE@3" direction="pwr"/>
<pin name="VDDCORE@4" direction="pwr"/>
<pin name="VDDCORE@5" direction="pwr"/>
<pin name="VDDCORE@6" direction="pwr"/>
<pin name="VDDCORE@7" direction="pwr"/>
<pin name="VDDCORE@8" direction="pwr"/>
<pin name="VDDCORE@9" direction="pwr"/>
<pin name="VDDCORE@10" direction="pwr"/>
<pin name="VDDRING@1" direction="pwr"/>
<pin name="VDDRING@2" direction="pwr"/>
<pin name="VDDRING@3" direction="pwr"/>
<pin name="VDDRING@4" direction="pwr"/>
<pin name="VDDRING@5" direction="pwr"/>
<pin name="VDDRING@6" direction="pwr"/>
<pin name="VDDRING@7" direction="pwr"/>
<pin name="VDDRING@8" direction="pwr"/>
<pin name="VDDRING@9" direction="pwr"/>
<pin name="VDDRING@10" direction="pwr"/>
<pin name="VSSCORE" direction="pwr"/>
<pin name="VSSCORE@1" direction="pwr"/>
<pin name="VSSCORE@2" direction="pwr"/>
<pin name="VSSCORE@3" direction="pwr"/>
<pin name="VSSCORE@4" direction="pwr"/>
<pin name="VSSCORE@5" direction="pwr"/>
<pin name="VSSCORE@6" direction="pwr"/>
<pin name="VSSCORE@7" direction="pwr"/>
<pin name="VSSRING@1" direction="pwr"/>
<pin name="VSSRING@2" direction="pwr"/>
<pin name="VSSRING@3" direction="pwr"/>
<pin name="VSSRING@4" direction="pwr"/>
<pin name="VSSRING@5" direction="pwr"/>
<pin name="VSSRING@6" direction="pwr"/>
<pin name="VSSRING@7" direction="pwr"/>
<pin name="VSSRING@8" direction="pwr"/>
</symbol>
<symbol name="ADUC70XX">
<pin name="ADC0" direction="in"/>
<pin name="ADC1" direction="in"/>
<pin name="ADC2/CMP0" direction="in"/>
<pin name="ADC3/CMP1" direction="in"/>
<pin name="ADC4" direction="in"/>
<pin name="ADC5" direction="in"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="ADC8" direction="in"/>
<pin name="ADC9" direction="in"/>
<pin name="ADC10" direction="in"/>
<pin name="ADC11" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="!RST" direction="in"/>
<pin name="XCLKI" direction="in"/>
<pin name="XCLKO" direction="out"/>
<pin name="DAC0/ADC12" direction="in"/>
<pin name="DAC1/ADC13" direction="in"/>
<pin name="DAC2/ADC14" direction="in"/>
<pin name="DAC3/ADC15" direction="in"/>
<pin name="P3.0/AD0/PWM0H" direction="out"/>
<pin name="P3.1/AD1/PWM0L" direction="out"/>
<pin name="P3.2/AD2/PWM1H" direction="out"/>
<pin name="P3.3/AD3/PWM1L" direction="out"/>
<pin name="P3.4/AD4/PWM2H" direction="out"/>
<pin name="P3.5/AD5/PWM2L" direction="out"/>
<pin name="GNDREF" direction="in"/>
<pin name="REFGND" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="IOGND" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="IOGND@1" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="LVDD" direction="out"/>
<pin name="DACVDD" direction="pwr"/>
<pin name="DACGND" direction="pwr"/>
<pin name="DACREF" direction="in"/>
<pin name="P3.6/AD6/PWMTRIP" direction="out"/>
<pin name="P3.7/AD7/PWMSYNC" direction="out"/>
<pin name="P0.7/ECLK/XCLK"/>
<pin name="P0.4/IRQ0"/>
<pin name="P0.5/IRQ1"/>
<pin name="P0.1/!BLE"/>
<pin name="P0.2/!BHE"/>
<pin name="P0.3/TRST/A16"/>
<pin name="P0.6/T1/MRST/AE"/>
<pin name="P0.0/BM/CMPOUT/MS2"/>
<pin name="P2.0/SPM9/!CONVSTART"/>
<pin name="P2.1/!WS"/>
<pin name="P2.2/!RS"/>
<pin name="P2.3/AE"/>
<pin name="P2.4/MS0"/>
<pin name="P2.5/MS1"/>
<pin name="P2.6/MS2"/>
<pin name="P2.7/MS3"/>
<pin name="P4.0/AD8"/>
<pin name="P4.1/AD9"/>
<pin name="P4.2/AD10"/>
<pin name="P4.3/AD11"/>
<pin name="P4.4/AD12"/>
<pin name="P4.5/AD13"/>
<pin name="P4.6/AD14"/>
<pin name="P4.7/AD15"/>
<pin name="P1.0/T1/SPM0"/>
<pin name="P1.1/SPM1"/>
<pin name="P1.2/SPM2"/>
<pin name="P1.3/SPM3"/>
<pin name="P1.4/SPM4/IRQ2"/>
<pin name="P1.5/SPM5/IRQ3"/>
<pin name="P1.6/SPM6"/>
<pin name="P1.7/SPM7"/>
<pin name="ADCNEG" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="ADUC7019">
<pin name="ADC0" direction="in"/>
<pin name="ADC1" direction="in"/>
<pin name="ADC2/CMP0" direction="in"/>
<pin name="ADC3/CMP1" direction="in"/>
<pin name="ADC4" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="!RST" direction="in"/>
<pin name="XCLKI" direction="in"/>
<pin name="XCLKO" direction="out"/>
<pin name="DAC0/ADC12" direction="in"/>
<pin name="DAC1/ADC13" direction="in"/>
<pin name="DAC2/ADC14" direction="in"/>
<pin name="DAC3/ADC15" direction="in"/>
<pin name="GNDREF" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="IOGND" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="LVDD" direction="out"/>
<pin name="P0.7/ECLK/XCLK"/>
<pin name="P0.4/IRQ0"/>
<pin name="P0.5/IRQ1"/>
<pin name="P0.3/TRST/A16"/>
<pin name="P0.6/T1/MRST/AE"/>
<pin name="P0.0/BM/CMPOUT/MS2"/>
<pin name="P2.0/SPM9/!CONVSTART"/>
<pin name="P1.0/T1/SPM0"/>
<pin name="P1.1/SPM1"/>
<pin name="P1.2/SPM2"/>
<pin name="P1.3/SPM3"/>
<pin name="P1.4/SPM4/IRQ2"/>
<pin name="P1.5/SPM5/IRQ3"/>
<pin name="P1.6/SPM6"/>
<pin name="P1.7/SPM7"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="P4.2"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="ADUC7021">
<pin name="ADC0" direction="in"/>
<pin name="ADC1" direction="in"/>
<pin name="ADC2/CMP0" direction="in"/>
<pin name="ADC3/CMP1" direction="in"/>
<pin name="ADC4" direction="in"/>
<pin name="ADC5" direction="in"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="!RST" direction="in"/>
<pin name="XCLKI" direction="in"/>
<pin name="XCLKO" direction="out"/>
<pin name="DAC0/ADC12" direction="in"/>
<pin name="DAC1/ADC13" direction="in"/>
<pin name="GNDREF" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="IOGND" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="LVDD" direction="out"/>
<pin name="P0.7/ECLK/XCLK"/>
<pin name="P0.4/IRQ0"/>
<pin name="P0.5/IRQ1"/>
<pin name="P0.3/TRST/A16"/>
<pin name="P0.6/T1/MRST/AE"/>
<pin name="P2.0/SPM9/!CONVSTART"/>
<pin name="P1.0/T1/SPM0"/>
<pin name="P1.1/SPM1"/>
<pin name="P1.2/SPM2"/>
<pin name="P1.3/SPM3"/>
<pin name="P1.4/SPM4/IRQ2"/>
<pin name="P1.5/SPM5/IRQ3"/>
<pin name="P1.6/SPM6"/>
<pin name="P1.7/SPM7"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="EXP" direction="pas"/>
<pin name="P0.0/BM/CMPOUT"/>
</symbol>
<symbol name="ADUC7022">
<pin name="ADC0" direction="in"/>
<pin name="ADC1" direction="in"/>
<pin name="ADC2/CMP0" direction="in"/>
<pin name="ADC3/CMP1" direction="in"/>
<pin name="ADC4" direction="in"/>
<pin name="ADC5" direction="in"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="ADC8" direction="in"/>
<pin name="ADC9" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="!RST" direction="in"/>
<pin name="XCLKI" direction="in"/>
<pin name="XCLKO" direction="out"/>
<pin name="GNDREF" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="IOGND" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="LVDD" direction="out"/>
<pin name="P0.7/ECLK/XCLK"/>
<pin name="P0.4/IRQ0"/>
<pin name="P0.5/IRQ1"/>
<pin name="P0.3/TRST/A16"/>
<pin name="P0.6/T1/MRST/AE"/>
<pin name="P0.0/BM/CMPOUT/MS2"/>
<pin name="P2.0/SPM9/!CONVSTART"/>
<pin name="P1.0/T1/SPM0"/>
<pin name="P1.1/SPM1"/>
<pin name="P1.2/SPM2"/>
<pin name="P1.3/SPM3"/>
<pin name="P1.4/SPM4/IRQ2"/>
<pin name="P1.5/SPM5/IRQ3"/>
<pin name="P1.6/SPM6"/>
<pin name="P1.7/SPM7"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="ADUC7024">
<pin name="ADC0" direction="in"/>
<pin name="ADC1" direction="in"/>
<pin name="ADC2/CMP0" direction="in"/>
<pin name="ADC3/CMP1" direction="in"/>
<pin name="ADC4" direction="in"/>
<pin name="ADC5" direction="in"/>
<pin name="ADC6" direction="in"/>
<pin name="ADC7" direction="in"/>
<pin name="ADC8" direction="in"/>
<pin name="ADC9" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="!RST" direction="in"/>
<pin name="XCLKI" direction="in"/>
<pin name="XCLKO" direction="out"/>
<pin name="DAC0/ADC12" direction="in"/>
<pin name="DAC1/ADC13" direction="in"/>
<pin name="P3.0/AD0/PWM0H" direction="out"/>
<pin name="P3.1/AD1/PWM0L" direction="out"/>
<pin name="P3.2/AD2/PWM1H" direction="out"/>
<pin name="P3.3/AD3/PWM1L" direction="out"/>
<pin name="P3.4/AD4/PWM2H" direction="out"/>
<pin name="P3.5/AD5/PWM2L" direction="out"/>
<pin name="GNDREF" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="IOGND" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="IOGND@1" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="LVDD" direction="out"/>
<pin name="DACVDD" direction="pwr"/>
<pin name="DACGND" direction="pwr"/>
<pin name="P3.6/AD6/PWMTRIP" direction="out"/>
<pin name="P3.7/AD7/PWMSYNC" direction="out"/>
<pin name="P0.7/ECLK/XCLK"/>
<pin name="P0.4/IRQ0"/>
<pin name="P0.5/IRQ1"/>
<pin name="P0.3/TRST/A16"/>
<pin name="P0.6/T1/MRST/AE"/>
<pin name="P0.0/BM/CMPOUT/MS2"/>
<pin name="P2.0/SPM9/!CONVSTART"/>
<pin name="P4.0/AD8"/>
<pin name="P4.1/AD9"/>
<pin name="P4.2/AD10"/>
<pin name="P4.3/AD11"/>
<pin name="P4.4/AD12"/>
<pin name="P4.5/AD13"/>
<pin name="P4.6/AD14"/>
<pin name="P4.7/AD15"/>
<pin name="P1.0/T1/SPM0"/>
<pin name="P1.1/SPM1"/>
<pin name="P1.2/SPM2"/>
<pin name="P1.3/SPM3"/>
<pin name="P1.4/SPM4/IRQ2"/>
<pin name="P1.5/SPM5/IRQ3"/>
<pin name="P1.6/SPM6"/>
<pin name="P1.7/SPM7"/>
<pin name="ADCNEG" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DACREF" direction="in"/>
</symbol>
<symbol name="AD8611">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="L" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AD8612">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!OUT" direction="out"/>
<pin name="L" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AD8367">
<pin name="ICOM@1" direction="pwr"/>
<pin name="ICOM@2" direction="pwr"/>
<pin name="OCOM" direction="pwr"/>
<pin name="ICOM@3" direction="pwr"/>
<pin name="VPSI" direction="pwr"/>
<pin name="VPSO" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="DECL" direction="out"/>
<pin name="HPFL" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="IN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="GAIN" direction="in"/>
<pin name="DETO" direction="out"/>
</symbol>
<symbol name="AD7142">
<pin name="CIN0" direction="in"/>
<pin name="CIN1" direction="in"/>
<pin name="CIN2" direction="in"/>
<pin name="CIN3" direction="in"/>
<pin name="CIN4" direction="in"/>
<pin name="CIN5" direction="in"/>
<pin name="CIN6" direction="in"/>
<pin name="CIN7" direction="in"/>
<pin name="CIN8" direction="in"/>
<pin name="CIN9" direction="in"/>
<pin name="CIN10" direction="in"/>
<pin name="CIN11" direction="in"/>
<pin name="CIN12" direction="in"/>
<pin name="CIN13" direction="in"/>
<pin name="CSHIELD" direction="out"/>
<pin name="SRC" direction="in"/>
<pin name="!SRC" direction="in"/>
<pin name="VDRIVE" direction="in"/>
<pin name="SDO/SDA" direction="out"/>
<pin name="SDI/ADD0"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS!/ADD1" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="GPIO" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="AVCC" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="VCC@D" direction="pwr"/>
<pin name="GND@D1" direction="pwr"/>
<pin name="GND@D2" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="AD7992">
<pin name="VIN1" direction="in"/>
<pin name="VIN2" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="AS" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="ALERT" direction="out"/>
<pin name="!CONVST" direction="in"/>
<pin name="AGND@1" direction="pwr"/>
</symbol>
<symbol name="ADSP_BF561_256_MBGA">
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="ADDR20" direction="out"/>
<pin name="ADDR21" direction="out"/>
<pin name="ADDR22" direction="out"/>
<pin name="ADDR23" direction="out"/>
<pin name="ADDR24" direction="out"/>
<pin name="ADDR25" direction="out"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="DATA16"/>
<pin name="DATA17"/>
<pin name="DATA18"/>
<pin name="DATA19"/>
<pin name="DATA20"/>
<pin name="DATA21"/>
<pin name="DATA22"/>
<pin name="DATA23"/>
<pin name="DATA24"/>
<pin name="DATA25"/>
<pin name="DATA26"/>
<pin name="DATA27"/>
<pin name="DATA28"/>
<pin name="DATA29"/>
<pin name="DATA30"/>
<pin name="DATA31"/>
<pin name="AMS_B0" direction="out"/>
<pin name="AMS_B1" direction="out"/>
<pin name="AMS_B2" direction="out"/>
<pin name="AMS_B3" direction="out"/>
<pin name="AOE_B" direction="out"/>
<pin name="ARDY" direction="in"/>
<pin name="ARE_B" direction="out"/>
<pin name="AWE_B" direction="out"/>
<pin name="ABE_B0" direction="out"/>
<pin name="ABE_B1" direction="out"/>
<pin name="ABE_B2" direction="out"/>
<pin name="ABE_B3" direction="out"/>
<pin name="BG_B" direction="out"/>
<pin name="BGH_B" direction="out"/>
<pin name="BY_PASS" direction="in"/>
<pin name="SLEEP" direction="out"/>
<pin name="BMODE0" direction="in"/>
<pin name="BMODE1" direction="in"/>
<pin name="BR_B" direction="in"/>
<pin name="DR0PRI"/>
<pin name="DR0SEC"/>
<pin name="DR1PRI"/>
<pin name="DR1SEC"/>
<pin name="DT0PRI"/>
<pin name="DT0SEC"/>
<pin name="DT1PRI"/>
<pin name="DT1SEC"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="NMI_0" direction="in"/>
<pin name="NMI_1" direction="in"/>
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PF8"/>
<pin name="PF9"/>
<pin name="PF10"/>
<pin name="PF11"/>
<pin name="PF12"/>
<pin name="PF13"/>
<pin name="PF14"/>
<pin name="PF15"/>
<pin name="PPI1_CLK" direction="in"/>
<pin name="PPI2_CLK" direction="in"/>
<pin name="PPI1_DATA0"/>
<pin name="PPI1_DATA1"/>
<pin name="PPI1_DATA2"/>
<pin name="PPI1_DATA3"/>
<pin name="PPI1_DATA4"/>
<pin name="PPI1_DATA5"/>
<pin name="PPI1_DATA6"/>
<pin name="PPI1_DATA7"/>
<pin name="PPI1_DATA8"/>
<pin name="PPI1_DATA9"/>
<pin name="PPI1_DATA10"/>
<pin name="PPI1_DATA11"/>
<pin name="PPI1_DATA12"/>
<pin name="PPI1_DATA13"/>
<pin name="PPI1_DATA14"/>
<pin name="PPI1_DATA15"/>
<pin name="PPI1_SYNC1"/>
<pin name="PPI1_SYNC2"/>
<pin name="PPI1_SYNC3"/>
<pin name="PPI2_DATA0"/>
<pin name="PPI2_DATA1"/>
<pin name="PPI2_DATA2"/>
<pin name="PPI2_DATA3"/>
<pin name="PPI2_DATA4"/>
<pin name="PPI2_DATA5"/>
<pin name="PPI2_DATA6"/>
<pin name="PPI2_DATA7"/>
<pin name="PPI2_DATA8"/>
<pin name="PPI2_DATA9"/>
<pin name="PPI2_DATA10"/>
<pin name="PPI2_DATA11"/>
<pin name="PPI2_DATA12"/>
<pin name="PPI2_DATA13"/>
<pin name="PPI2_DATA14"/>
<pin name="PPI2_DATA15"/>
<pin name="PPI2_SYNC1"/>
<pin name="PPI2_SYNC2"/>
<pin name="PPI2_SYNC3"/>
<pin name="RFS0"/>
<pin name="RFS1"/>
<pin name="RESET_B" direction="in"/>
<pin name="RSCLK0"/>
<pin name="RSCLK1"/>
<pin name="TSCLK0"/>
<pin name="TSCLK1"/>
<pin name="RX"/>
<pin name="TX"/>
<pin name="SA10" direction="out"/>
<pin name="SCAS_B" direction="out"/>
<pin name="SCK"/>
<pin name="SCKE" direction="out"/>
<pin name="SMS_B0" direction="out"/>
<pin name="SMS_B1" direction="out"/>
<pin name="SMS_B2" direction="out"/>
<pin name="SMS_B3" direction="out"/>
<pin name="SRAS_B" direction="out"/>
<pin name="SWE_B" direction="out"/>
<pin name="SCLK0" direction="out"/>
<pin name="SCLK1" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="EMU_B" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="TFS0"/>
<pin name="TFS1"/>
<pin name="TRST_B" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="VDD_INT@0" direction="pwr"/>
<pin name="VDD_INT@1" direction="pwr"/>
<pin name="VDD_INT@2" direction="pwr"/>
<pin name="VDD_INT@3" direction="pwr"/>
<pin name="VDD_INT@4" direction="pwr"/>
<pin name="VDD_INT@5" direction="pwr"/>
<pin name="VDD_INT@6" direction="pwr"/>
<pin name="VDD_INT@7" direction="pwr"/>
<pin name="VDD_INT@8" direction="pwr"/>
<pin name="GND_INT@0" direction="pwr"/>
<pin name="GND_INT@1" direction="pwr"/>
<pin name="GND_INT@2" direction="pwr"/>
<pin name="GND_INT@3" direction="pwr"/>
<pin name="GND_INT@4" direction="pwr"/>
<pin name="GND_INT@5" direction="pwr"/>
<pin name="GND_INT@6" direction="pwr"/>
<pin name="VDD_EXT@0" direction="pwr"/>
<pin name="VDD_EXT@1" direction="pwr"/>
<pin name="VDD_EXT@2" direction="pwr"/>
<pin name="VDD_EXT@3" direction="pwr"/>
<pin name="VDD_EXT@4" direction="pwr"/>
<pin name="VDD_EXT@5" direction="pwr"/>
<pin name="VDD_EXT@6" direction="pwr"/>
<pin name="VDD_EXT@7" direction="pwr"/>
<pin name="VDD_EXT@8" direction="pwr"/>
<pin name="VDD_EXT@9" direction="pwr"/>
<pin name="VDD_EXT@10" direction="pwr"/>
<pin name="VDD_EXT@11" direction="pwr"/>
<pin name="VDD_EXT@12" direction="pwr"/>
<pin name="VDD_EXT@13" direction="pwr"/>
<pin name="VDD_EXT@14" direction="pwr"/>
<pin name="VDD_EXT@15" direction="pwr"/>
<pin name="VDD_EXT@16" direction="pwr"/>
<pin name="VDD_EXT@17" direction="pwr"/>
<pin name="VDD_EXT@18" direction="pwr"/>
<pin name="GND_EXT@0" direction="pwr"/>
<pin name="GND_EXT@1" direction="pwr"/>
<pin name="GND_EXT@2" direction="pwr"/>
<pin name="GND_EXT@3" direction="pwr"/>
<pin name="GND_EXT@4" direction="pwr"/>
<pin name="GND_EXT@5" direction="pwr"/>
<pin name="GND_EXT@6" direction="pwr"/>
<pin name="GND_EXT@7" direction="pwr"/>
<pin name="GND_EXT@8" direction="pwr"/>
<pin name="GND_EXT@9" direction="pwr"/>
<pin name="GND_EXT@10" direction="pwr"/>
<pin name="GND_EXT@11" direction="pwr"/>
<pin name="GND_EXT@12" direction="pwr"/>
<pin name="GND_EXT@13" direction="pwr"/>
<pin name="GND_EXT@14" direction="pwr"/>
<pin name="GND_EXT@15" direction="pwr"/>
<pin name="GND_EXT@16" direction="pwr"/>
<pin name="GND_EXT@17" direction="pwr"/>
<pin name="GND_EXT@18" direction="pwr"/>
<pin name="CLKIN" direction="in"/>
<pin name="XTAL" direction="out"/>
<pin name="VREF_FLT" direction="in"/>
<pin name="VREG" direction="in"/>
<pin name="PSMON_VDD" direction="pwr"/>
<pin name="PSMON_GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="VDD_INT@9" direction="pwr"/>
<pin name="VDD_INT@10" direction="pwr"/>
<pin name="VDD_INT@11" direction="pwr"/>
<pin name="VDD_INT@12" direction="pwr"/>
<pin name="VDD_INT@13" direction="pwr"/>
<pin name="VDD_EXT@19" direction="pwr"/>
<pin name="VDD_EXT@20" direction="pwr"/>
<pin name="VDD_EXT@21" direction="pwr"/>
<pin name="VDD_EXT@22" direction="pwr"/>
</symbol>
<symbol name="OP+-VS">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="-VS" direction="in"/>
<pin name="+VS" direction="in"/>
</symbol>
<symbol name="AD7714">
<pin name="MCLKOUT" direction="out"/>
<pin name="!SYNC" direction="in"/>
<pin name="BUFFER" direction="in"/>
<pin name="POL" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="REFIN+" direction="in"/>
<pin name="REFIN-" direction="in"/>
<pin name="!DRDY" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="DVDD" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="MCLKIN" direction="in"/>
<pin name="DGND" direction="in"/>
<pin name="!STANDBY" direction="in"/>
</symbol>
<symbol name="AD421">
<pin name="DRIVE" direction="out"/>
<pin name="BOOST" direction="oc"/>
<pin name="DATA" direction="in"/>
<pin name="LOOP-RTN" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="REFIN" direction="in"/>
<pin name="REFOUT1" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="COM" direction="pwr"/>
<pin name="COMP" direction="out"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="CLOCK" direction="in"/>
<pin name="LATCH" direction="in"/>
<pin name="REFOUT2" direction="out"/>
<pin name="LV" direction="in"/>
</symbol>
<symbol name="AD9859">
<pin name="I/O_UPDATE" direction="in"/>
<pin name="DVDD@1" direction="in"/>
<pin name="DVDD@2" direction="in"/>
<pin name="DGND@1" direction="in"/>
<pin name="DGND@2" direction="in"/>
<pin name="DGND@3" direction="in"/>
<pin name="DGND@4" direction="in"/>
<pin name="DGND@5" direction="in"/>
<pin name="AVDD@1" direction="in"/>
<pin name="AVDD@2" direction="in"/>
<pin name="AVDD@3" direction="in"/>
<pin name="AVDD@4" direction="in"/>
<pin name="AVDD@5" direction="in"/>
<pin name="AVDD@6" direction="in"/>
<pin name="AVDD@7" direction="in"/>
<pin name="AVDD@8" direction="in"/>
<pin name="AVDD@9" direction="in"/>
<pin name="AGND@1" direction="in"/>
<pin name="AGND@2" direction="in"/>
<pin name="AGND@3" direction="in"/>
<pin name="AGND@4" direction="in"/>
<pin name="AGND@5" direction="in"/>
<pin name="AGND@6" direction="in"/>
<pin name="AGND@7" direction="in"/>
<pin name="AGND@8" direction="in"/>
<pin name="AGND@9" direction="in"/>
<pin name="!OSC/!REFCLK" direction="in"/>
<pin name="OSC/REFCLK" direction="in"/>
<pin name="CRYSTAL_OUT" direction="out"/>
<pin name="CLKMODESELECT" direction="in"/>
<pin name="LOOP_FILTER" direction="in"/>
<pin name="!IOUT" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="DACBP" direction="in"/>
<pin name="DAC_RSET" direction="in"/>
<pin name="PWRDWNCTL" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="IOSYNC" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="!CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDIO"/>
<pin name="DVDD_I/O" direction="in"/>
<pin name="SYNC_IN" direction="in"/>
<pin name="SYNC_CLK" direction="out"/>
<pin name="OSK" direction="in"/>
<pin name="AGND@11" direction="in"/>
<pin name="AGND@10" direction="in"/>
<pin name="AGND/EXP" direction="in"/>
</symbol>
<symbol name="AD7651">
<pin name="AGND" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="INGND" direction="in"/>
<pin name="PDREF" direction="in"/>
<pin name="PDBUF" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="OVDD" direction="in"/>
<pin name="OGND" direction="in"/>
<pin name="DVDD" direction="in"/>
<pin name="DGND" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="BUSY" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="D12" direction="in"/>
<pin name="D13" direction="in"/>
<pin name="D14" direction="in"/>
<pin name="D15" direction="in"/>
<pin name="OB/!2C" direction="in"/>
<pin name="BYTESWAP" direction="in"/>
<pin name="!CNVST" direction="in"/>
<pin name="REFBUFIN" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="REFGND" direction="in"/>
<pin name="SER/!PAR" direction="in"/>
<pin name="AGND@EXP" direction="in"/>
<pin name="AGND@1" direction="in"/>
<pin name="AGND@2" direction="in"/>
<pin name="AGND@3" direction="in"/>
<pin name="DGND@1" direction="in"/>
<pin name="AVDD@1" direction="in"/>
<pin name="TEMP" direction="in"/>
</symbol>
<symbol name="ADG419">
<pin name="D"/>
<pin name="S1"/>
<pin name="S2"/>
<pin name="IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VL" direction="pwr"/>
</symbol>
<symbol name="AD620">
<pin name="+" direction="in"/>
<pin name="-" direction="in"/>
<pin name="-V" direction="pwr"/>
<pin name="+V" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="RG@1" direction="pas"/>
<pin name="RG@2" direction="pas"/>
<pin name="REF" direction="pas"/>
</symbol>
<symbol name="AD8353">
<pin name="RFIN" direction="in"/>
<pin name="COM1@1" direction="in"/>
<pin name="COM2@1" direction="in"/>
<pin name="RFOUT" direction="out"/>
<pin name="VPOS" direction="pwr"/>
<pin name="COM1@2" direction="in"/>
<pin name="COM2@2" direction="in"/>
<pin name="EXP@2" direction="in"/>
<pin name="EXP@1" direction="in"/>
</symbol>
<symbol name="AD780">
<pin name="+VIN" direction="in"/>
<pin name="TEMP" direction="in"/>
<pin name="TRIM" direction="in"/>
<pin name="VOUT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="O/P" direction="pas"/>
</symbol>
<symbol name="AD9901">
<pin name="REFIN" direction="out"/>
<pin name="OUT" direction="in"/>
<pin name="!OUT" direction="in"/>
<pin name="BIAS" direction="in"/>
<pin name="VCOIN" direction="in"/>
<pin name="RSET" direction="in"/>
<pin name="+VS@1" direction="in"/>
<pin name="+VS@2" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="GND@3" direction="in"/>
<pin name="GND@4" direction="in"/>
<pin name="GND@5" direction="in"/>
<pin name="GND@6" direction="in"/>
</symbol>
<symbol name="AD7303">
<pin name="DIN" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!SYNC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VREF" direction="pas"/>
<pin name="VOUTA" direction="out"/>
<pin name="VOUTB" direction="out"/>
</symbol>
<symbol name="AD9951">
<pin name="I/O_UPDATE" direction="in"/>
<pin name="SYNC_CLK" direction="out"/>
<pin name="REFCLK" direction="in"/>
<pin name="!REFCLK" direction="in"/>
<pin name="CRYSTAL_OUT" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="!IOUT" direction="out"/>
<pin name="DAC_RSET" direction="in"/>
<pin name="SYNC_IN" direction="in"/>
<pin name="OSK" direction="in"/>
<pin name="PWRDWNCTL" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLKMODESELCT" direction="in"/>
<pin name="LOOP_FILTER" direction="in"/>
<pin name="DACBP" direction="in"/>
<pin name="IOSYNC" direction="in"/>
<pin name="SDO" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDIO"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DGND@4" direction="pwr"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="AVDD@4" direction="pwr"/>
<pin name="AVDD@5" direction="pwr"/>
<pin name="AVDD@6" direction="pwr"/>
<pin name="AVDD@7" direction="pwr"/>
<pin name="AVDD@8" direction="pwr"/>
<pin name="AVDD@9" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AGND@5" direction="pwr"/>
<pin name="AGND@6" direction="pwr"/>
<pin name="AGND@7" direction="pwr"/>
<pin name="AGND@8" direction="pwr"/>
<pin name="AGND@9" direction="pwr"/>
<pin name="AGND@10" direction="pwr"/>
<pin name="AGND@11" direction="pwr"/>
<pin name="DVDD_I/O" direction="pwr"/>
<pin name="DGND@5" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="17303025021367_256BALLSBGA_BSDL_PRA_0106">
<pin name="ACK" direction="in"/>
<pin name="BOOTCFG0" direction="in"/>
<pin name="BOOTCFG1" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLK_CFG0" direction="in"/>
<pin name="CLK_CFG1" direction="in"/>
<pin name="GND_0" direction="in"/>
<pin name="GND_1" direction="in"/>
<pin name="GND_2" direction="in"/>
<pin name="NC_6" direction="in"/>
<pin name="RESET_B" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="DAI1"/>
<pin name="DAI2"/>
<pin name="DAI3"/>
<pin name="DAI4"/>
<pin name="DAI5"/>
<pin name="DAI6"/>
<pin name="DAI7"/>
<pin name="DAI8"/>
<pin name="DAI9"/>
<pin name="DAI10"/>
<pin name="DAI11"/>
<pin name="DAI12"/>
<pin name="DAI13"/>
<pin name="DAI14"/>
<pin name="DAI15"/>
<pin name="DAI16"/>
<pin name="DAI17"/>
<pin name="DAI18"/>
<pin name="DAI19"/>
<pin name="DAI20"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="DATA16"/>
<pin name="DATA17"/>
<pin name="DATA18"/>
<pin name="DATA19"/>
<pin name="DATA20"/>
<pin name="DATA21"/>
<pin name="DATA22"/>
<pin name="DATA23"/>
<pin name="DATA24"/>
<pin name="DATA25"/>
<pin name="DATA26"/>
<pin name="DATA27"/>
<pin name="DATA28"/>
<pin name="DATA29"/>
<pin name="DATA30"/>
<pin name="DATA31"/>
<pin name="DPI1"/>
<pin name="DPI2"/>
<pin name="DPI3"/>
<pin name="DPI4"/>
<pin name="DPI5"/>
<pin name="DPI6"/>
<pin name="DPI7"/>
<pin name="DPI8"/>
<pin name="DPI9"/>
<pin name="DPI10"/>
<pin name="DPI11"/>
<pin name="DPI12"/>
<pin name="DPI13"/>
<pin name="DPI14"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="NC_1"/>
<pin name="NC_2"/>
<pin name="NC_3"/>
<pin name="NC_4"/>
<pin name="NC_5"/>
<pin name="SDCLK0"/>
<pin name="ADDR0" direction="out"/>
<pin name="ADDR1" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="ADDR20" direction="out"/>
<pin name="ADDR21" direction="out"/>
<pin name="ADDR22" direction="out"/>
<pin name="ADDR23" direction="out"/>
<pin name="CLKOUT" direction="out"/>
<pin name="EMU_B" direction="out"/>
<pin name="MS0_B" direction="out"/>
<pin name="MS1_B" direction="out"/>
<pin name="RD_B" direction="out"/>
<pin name="SDA10" direction="out"/>
<pin name="SDCAS_B" direction="out"/>
<pin name="SDCKE" direction="out"/>
<pin name="SDRAS_B" direction="out"/>
<pin name="SDWE_B" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="WR_B" direction="out"/>
<pin name="XTAL" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="VDD@31" direction="pwr"/>
<pin name="VDD@32" direction="pwr"/>
<pin name="VDD@33" direction="pwr"/>
<pin name="VDD@34" direction="pwr"/>
<pin name="IOVDD@0" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="IOVDD@2" direction="pwr"/>
<pin name="IOVDD@3" direction="pwr"/>
<pin name="IOVDD@4" direction="pwr"/>
<pin name="IOVDD@5" direction="pwr"/>
<pin name="IOVDD@6" direction="pwr"/>
<pin name="IOVDD@7" direction="pwr"/>
<pin name="IOVDD@8" direction="pwr"/>
<pin name="IOVDD@9" direction="pwr"/>
<pin name="IOVDD@10" direction="pwr"/>
<pin name="IOVDD@11" direction="pwr"/>
<pin name="IOVDD@12" direction="pwr"/>
<pin name="IOVDD@13" direction="pwr"/>
<pin name="IOVDD@14" direction="pwr"/>
<pin name="IOVDD@15" direction="pwr"/>
<pin name="IOVDD@16" direction="pwr"/>
<pin name="IOVDD@17" direction="pwr"/>
<pin name="IOVDD@18" direction="pwr"/>
<pin name="IOVDD@19" direction="pwr"/>
<pin name="IOVDD@20" direction="pwr"/>
<pin name="IOVDD@21" direction="pwr"/>
<pin name="IOVDD@22" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="GND@37" direction="pwr"/>
<pin name="GND@38" direction="pwr"/>
<pin name="GND@39" direction="pwr"/>
<pin name="GND@40" direction="pwr"/>
<pin name="GND@41" direction="pwr"/>
<pin name="GND@42" direction="pwr"/>
<pin name="GND@43" direction="pwr"/>
<pin name="GND@44" direction="pwr"/>
<pin name="GND@45" direction="pwr"/>
<pin name="GND@46" direction="pwr"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@48" direction="pwr"/>
<pin name="GND@49" direction="pwr"/>
<pin name="GND@50" direction="pwr"/>
<pin name="GND@51" direction="pwr"/>
<pin name="GND@52" direction="pwr"/>
<pin name="GND@53" direction="pwr"/>
<pin name="GND@54" direction="pwr"/>
<pin name="GND@55" direction="pwr"/>
<pin name="GND@56" direction="pwr"/>
<pin name="GND@57" direction="pwr"/>
<pin name="NC0" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="NC5" direction="pas"/>
<pin name="NC6" direction="pas"/>
<pin name="NC7" direction="pas"/>
<pin name="NC8" direction="pas"/>
<pin name="NC9" direction="pas"/>
</symbol>
<symbol name="21367_208MQFP">
<pin name="ACK" direction="in"/>
<pin name="BOOTCFG0" direction="in"/>
<pin name="BOOTCFG1" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLK_CFG0" direction="in"/>
<pin name="CLK_CFG1" direction="in"/>
<pin name="RESET_B" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="DAI1"/>
<pin name="DAI2"/>
<pin name="DAI3"/>
<pin name="DAI4"/>
<pin name="DAI5"/>
<pin name="DAI6"/>
<pin name="DAI7"/>
<pin name="DAI8"/>
<pin name="DAI9"/>
<pin name="DAI10"/>
<pin name="DAI11"/>
<pin name="DAI12"/>
<pin name="DAI13"/>
<pin name="DAI14"/>
<pin name="DAI15"/>
<pin name="DAI16"/>
<pin name="DAI17"/>
<pin name="DAI18"/>
<pin name="DAI19"/>
<pin name="DAI20"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="DATA16"/>
<pin name="DATA17"/>
<pin name="DATA18"/>
<pin name="DATA19"/>
<pin name="DATA20"/>
<pin name="DATA21"/>
<pin name="DATA22"/>
<pin name="DATA23"/>
<pin name="DATA24"/>
<pin name="DATA25"/>
<pin name="DATA26"/>
<pin name="DATA27"/>
<pin name="DATA28"/>
<pin name="DATA29"/>
<pin name="DATA30"/>
<pin name="DATA31"/>
<pin name="DPI1"/>
<pin name="DPI2"/>
<pin name="DPI3"/>
<pin name="DPI4"/>
<pin name="DPI5"/>
<pin name="DPI6"/>
<pin name="DPI7"/>
<pin name="DPI8"/>
<pin name="DPI9"/>
<pin name="DPI10"/>
<pin name="DPI11"/>
<pin name="DPI12"/>
<pin name="DPI13"/>
<pin name="DPI14"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="SDCLK0"/>
<pin name="ADDR0" direction="out"/>
<pin name="ADDR1" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="ADDR20" direction="out"/>
<pin name="ADDR21" direction="out"/>
<pin name="ADDR22" direction="out"/>
<pin name="ADDR23" direction="out"/>
<pin name="CLKOUT" direction="out"/>
<pin name="EMU_B" direction="out"/>
<pin name="MS0_B" direction="out"/>
<pin name="MS1_B" direction="out"/>
<pin name="RD_B" direction="out"/>
<pin name="SDA10" direction="out"/>
<pin name="SDCAS_B" direction="out"/>
<pin name="SDCKE" direction="out"/>
<pin name="SDRAS_B" direction="out"/>
<pin name="SDWE_B" direction="out"/>
<pin name="TDO" direction="out"/>
<pin name="WR_B" direction="out"/>
<pin name="XTAL" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="IOVDD@0" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="IOVDD@2" direction="pwr"/>
<pin name="IOVDD@3" direction="pwr"/>
<pin name="IOVDD@4" direction="pwr"/>
<pin name="IOVDD@5" direction="pwr"/>
<pin name="IOVDD@6" direction="pwr"/>
<pin name="IOVDD@7" direction="pwr"/>
<pin name="IOVDD@8" direction="pwr"/>
<pin name="IOVDD@9" direction="pwr"/>
<pin name="IOVDD@10" direction="pwr"/>
<pin name="IOVDD@11" direction="pwr"/>
<pin name="IOVDD@12" direction="pwr"/>
<pin name="IOVDD@13" direction="pwr"/>
<pin name="IOVDD@14" direction="pwr"/>
<pin name="IOVDD@15" direction="pwr"/>
<pin name="IOVDD@16" direction="pwr"/>
<pin name="IOVDD@17" direction="pwr"/>
<pin name="IOVDD@18" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
</symbol>
<symbol name="ADIS16209">
<pin name="AUXADC" direction="in"/>
<pin name="AUXDAC" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="DIO1"/>
<pin name="DIO2"/>
<pin name="!RST" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ADG1408">
<pin name="S1"/>
<pin name="S2"/>
<pin name="S3"/>
<pin name="S4"/>
<pin name="S5"/>
<pin name="S6"/>
<pin name="S7"/>
<pin name="S8"/>
<pin name="D"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="ADG1409">
<pin name="S1A"/>
<pin name="S2A"/>
<pin name="S3A"/>
<pin name="S4A"/>
<pin name="DA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="S1B"/>
<pin name="S2B"/>
<pin name="S3B"/>
<pin name="S4B"/>
<pin name="DB"/>
</symbol>
<symbol name="PWR-VSS_GND_VDD_EXP">
<pin name="VSS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="PWR-VSS_GND_VDD">
<pin name="VSS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="ADG658">
<pin name="S1"/>
<pin name="S2"/>
<pin name="S3"/>
<pin name="S4"/>
<pin name="S5"/>
<pin name="S6"/>
<pin name="S7"/>
<pin name="S8"/>
<pin name="D"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!EN" direction="in"/>
</symbol>
<symbol name="ADG659">
<pin name="S1A"/>
<pin name="S2A"/>
<pin name="S3A"/>
<pin name="S4A"/>
<pin name="DA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!EN" direction="in"/>
<pin name="S1B"/>
<pin name="S2B"/>
<pin name="S3B"/>
<pin name="S4B"/>
<pin name="DB"/>
</symbol>
<symbol name="SSM2165">
<pin name="IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="BUFOUT" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="VCAIN" direction="in"/>
<pin name="AVGCAP" direction="pas"/>
<pin name="COMP" direction="pas"/>
</symbol>
<symbol name="SSM2166">
<pin name="+IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="BUFOUT" direction="out"/>
<pin name="VOUT" direction="out"/>
<pin name="VCAIN" direction="in"/>
<pin name="AVGCAP" direction="pas"/>
<pin name="COMP" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="VCAR" direction="in"/>
<pin name="VCA_GAIN_ADJ" direction="in"/>
<pin name="POWER_DOWN" direction="in"/>
<pin name="NOIS_GATE_SET" direction="pas"/>
<pin name="ROTATION_POINT_SET" direction="pas"/>
</symbol>
<symbol name="SSM2167">
<pin name="IN" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="BUFOUT" direction="out"/>
<pin name="OUTPUT" direction="out"/>
<pin name="VCAIN" direction="in"/>
<pin name="AVG_CAP" direction="pas"/>
<pin name="RCOMP" direction="pas"/>
<pin name="!SHUTDOWN" direction="in"/>
<pin name="RGATE" direction="pas"/>
</symbol>
<symbol name="AD1836">
<pin name="DVDD" direction="pwr"/>
<pin name="CDATA" direction="in"/>
<pin name="PD/RST" direction="in"/>
<pin name="OUTLP3" direction="out"/>
<pin name="OUTLN3" direction="out"/>
<pin name="OUTLP2" direction="out"/>
<pin name="OUTLN2" direction="out"/>
<pin name="OUTLP1" direction="out"/>
<pin name="OUTLN1" direction="out"/>
<pin name="AVDD" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="FILTD" direction="in"/>
<pin name="FILTR" direction="in"/>
<pin name="AGND@1" direction="in"/>
<pin name="AVDD@1" direction="in"/>
<pin name="ADC1INLP" direction="in"/>
<pin name="ADC1INLN" direction="in"/>
<pin name="ADC1INRP" direction="in"/>
<pin name="ADC1INRN" direction="in"/>
<pin name="ADC2INL+/CAPL2" direction="in"/>
<pin name="ADC2INL-/CAPL1" direction="in"/>
<pin name="ADC2INL1" direction="in"/>
<pin name="ADC2INL2" direction="in"/>
<pin name="ADC2INR2" direction="in"/>
<pin name="ADC2INR1" direction="in"/>
<pin name="ADC2INR-/CAPR1" direction="in"/>
<pin name="ADC2INR+/CAPR2" direction="in"/>
<pin name="AGND@2" direction="in"/>
<pin name="AGND@3" direction="in"/>
<pin name="OUTRN1" direction="out"/>
<pin name="OUTRP1" direction="out"/>
<pin name="OUTRN2" direction="out"/>
<pin name="OUTRP2" direction="out"/>
<pin name="OUTRN3" direction="out"/>
<pin name="OUTRP3" direction="out"/>
<pin name="DLRCLK"/>
<pin name="DBCLK"/>
<pin name="DSDATA1" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DSDATA2" direction="in"/>
<pin name="DSDATA3" direction="in"/>
<pin name="ABCLK" direction="out"/>
<pin name="ALRCLK" direction="out"/>
<pin name="MCLK" direction="in"/>
<pin name="ODVDD" direction="in"/>
<pin name="ASDATA1" direction="out"/>
<pin name="ASDATA2" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="CLATCH" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="DGND@1" direction="pwr"/>
</symbol>
<symbol name="ADUM1301">
<pin name="VDD1" direction="in"/>
<pin name="VDD2" direction="in"/>
<pin name="GND1@1" direction="in"/>
<pin name="GND2@1" direction="in"/>
<pin name="VIA" direction="in"/>
<pin name="VIB" direction="in"/>
<pin name="VIC" direction="in"/>
<pin name="GND1@2" direction="in"/>
<pin name="VOA" direction="hiz"/>
<pin name="VOB" direction="hiz"/>
<pin name="VOC" direction="hiz"/>
<pin name="VE2" direction="in"/>
<pin name="GND2@2" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="VE1" direction="in"/>
</symbol>
<symbol name="ADUM1300">
<pin name="VDD1" direction="in"/>
<pin name="VDD2" direction="in"/>
<pin name="GND1@1" direction="in"/>
<pin name="GND2@1" direction="in"/>
<pin name="VIA" direction="in"/>
<pin name="VIB" direction="in"/>
<pin name="VIC" direction="in"/>
<pin name="GND1@2" direction="in"/>
<pin name="VOA" direction="hiz"/>
<pin name="VOB" direction="hiz"/>
<pin name="VOC" direction="hiz"/>
<pin name="VE2" direction="in"/>
<pin name="GND2@2" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
</symbol>
<symbol name="AD1877">
<pin name="L!R!CK"/>
<pin name="WCLK"/>
<pin name="BCLK"/>
<pin name="DVDD1" direction="in"/>
<pin name="DGND1" direction="in"/>
<pin name="RDEDGE" direction="in"/>
<pin name="S/!M" direction="in"/>
<pin name="384/!256" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="VINL" direction="in"/>
<pin name="CAPL1" direction="out"/>
<pin name="CAPL2" direction="out"/>
<pin name="AGNDL" direction="in"/>
<pin name="VREFL" direction="out"/>
<pin name="VREFR" direction="out"/>
<pin name="AGNDR" direction="in"/>
<pin name="CAPR2" direction="out"/>
<pin name="CAPR1" direction="out"/>
<pin name="VINR" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="R!L!JUST" direction="in"/>
<pin name="!MSBDLY" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="DGND2" direction="in"/>
<pin name="DVDD2" direction="in"/>
<pin name="SOUT" direction="out"/>
<pin name="TAG" direction="out"/>
<pin name="CLKIN" direction="in"/>
</symbol>
<symbol name="AD1890">
<pin name="GPDLYS" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="DATA_I" direction="in"/>
<pin name="BCLK_I" direction="in"/>
<pin name="WCLK_I" direction="in"/>
<pin name="L!R!_I" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="N/C" direction="nc"/>
<pin name="BKPOL_I" direction="in"/>
<pin name="TRGLR_I" direction="in"/>
<pin name="MSBDLY_I" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="MUTE_I" direction="in"/>
<pin name="MUTE_O" direction="out"/>
<pin name="MSBDLY_O" direction="in"/>
<pin name="TRGLR_O" direction="in"/>
<pin name="BKPOL_O" direction="in"/>
<pin name="N/C@1" direction="nc"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="DATA_O" direction="out"/>
<pin name="L!R!_O" direction="in"/>
<pin name="WCLK_O" direction="in"/>
<pin name="BCLK_O" direction="in"/>
<pin name="GND@3" direction="pwr"/>
<pin name="SETLSLW" direction="in"/>
</symbol>
<symbol name="AD1891">
<pin name="N/C@1" direction="nc"/>
<pin name="MCLK" direction="in"/>
<pin name="DATA_I" direction="in"/>
<pin name="BCLK_I" direction="in"/>
<pin name="WCLK_I" direction="in"/>
<pin name="L!R!_I" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="N/C@2" direction="nc"/>
<pin name="BKPOL_I" direction="in"/>
<pin name="TRGLR_I" direction="in"/>
<pin name="MSBDLY_I" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="MUTE_I" direction="in"/>
<pin name="MUTE_O" direction="out"/>
<pin name="MSBDLY_O" direction="in"/>
<pin name="TRGLR_O" direction="in"/>
<pin name="BKPOL_O" direction="in"/>
<pin name="N/C@3" direction="nc"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="DATA_O" direction="out"/>
<pin name="L!R!_O" direction="in"/>
<pin name="WCLK_O" direction="in"/>
<pin name="BCLK_O" direction="in"/>
<pin name="GND@3" direction="pwr"/>
<pin name="SETLSLW" direction="in"/>
</symbol>
<symbol name="AD1892">
<pin name="PD/RST" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="QDFS" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="SFCLK" direction="out"/>
<pin name="U/CBIT" direction="out"/>
<pin name="INT" direction="out"/>
<pin name="ERROR" direction="out"/>
<pin name="NOSIG" direction="out"/>
<pin name="RXP" direction="in"/>
<pin name="RXN" direction="in"/>
<pin name="CON/PRO" direction="out"/>
<pin name="CSCLK" direction="out"/>
<pin name="CE" direction="out"/>
<pin name="CD" direction="out"/>
<pin name="CC" direction="out"/>
<pin name="CB" direction="out"/>
<pin name="CA" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="SDATA" direction="out"/>
<pin name="LRCLK" direction="out"/>
<pin name="BCLK" direction="out"/>
<pin name="MUTE" direction="in"/>
<pin name="MCLK" direction="in"/>
</symbol>
<symbol name="AD1953">
<pin name="NC" direction="nc"/>
<pin name="MCLK2" direction="in"/>
<pin name="MCLK1" direction="in"/>
<pin name="MCLK0" direction="in"/>
<pin name="AUXDATA" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SDATA2" direction="in"/>
<pin name="BCLK2" direction="in"/>
<pin name="LRCLK2" direction="in"/>
<pin name="SDATA1" direction="in"/>
<pin name="BCLK1" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="LRCLK1" direction="in"/>
<pin name="SDATA0" direction="in"/>
<pin name="BCLK0" direction="in"/>
<pin name="LRCLK0" direction="in"/>
<pin name="CDATA" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="CLATCH" direction="in"/>
<pin name="RESETB" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="VOUTS-" direction="out"/>
<pin name="VOUTS+" direction="out"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="VOUTR-" direction="out"/>
<pin name="VOUTR+" direction="out"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="VOUTL+" direction="out"/>
<pin name="VOUTL-" direction="out"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="VREF" direction="in"/>
<pin name="FILTCAP" direction="in"/>
<pin name="ZEROFLAG" direction="out"/>
<pin name="DMUXO/TDMO" direction="out"/>
<pin name="BMUXO/TDMBC" direction="out"/>
<pin name="LRMUXO/TDMFS" direction="out"/>
<pin name="ODVDD" direction="pwr"/>
<pin name="DCSOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="MCLKOUT" direction="out"/>
<pin name="DGND@1" direction="pwr"/>
</symbol>
<symbol name="AD1954">
<pin name="NC" direction="nc"/>
<pin name="MCLK2" direction="in"/>
<pin name="MCLK1" direction="in"/>
<pin name="MCLK0" direction="in"/>
<pin name="DEEMP/SDATA_AUX" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SDATA2" direction="in"/>
<pin name="BCLK2" direction="in"/>
<pin name="LRCLK2" direction="in"/>
<pin name="SDATA1" direction="in"/>
<pin name="BCLK1" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="LRCLK1" direction="in"/>
<pin name="SDATA0" direction="in"/>
<pin name="BCLK0" direction="in"/>
<pin name="LRCLK0" direction="in"/>
<pin name="CDATA" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="CLATCH" direction="in"/>
<pin name="RESETB" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="VOUTS-" direction="out"/>
<pin name="VOUTS+" direction="out"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="VOUTR-" direction="out"/>
<pin name="VOUTR+" direction="out"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="VOUTL+" direction="out"/>
<pin name="VOUTL-" direction="out"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="VREF" direction="in"/>
<pin name="FILTCAP" direction="in"/>
<pin name="ZEROFLAG" direction="out"/>
<pin name="SDATAOUT" direction="out"/>
<pin name="BCLKOUT" direction="out"/>
<pin name="LRCLKOUT" direction="out"/>
<pin name="ODVDD" direction="pwr"/>
<pin name="DCSOUT" direction="out"/>
<pin name="COUT" direction="out"/>
<pin name="MCLKOUT" direction="out"/>
<pin name="DGND@1" direction="pwr"/>
</symbol>
<symbol name="AD1983">
<pin name="NC" direction="nc"/>
<pin name="SDATA_OUT" direction="in"/>
<pin name="BIT_CLK" direction="in"/>
<pin name="DVSS" direction="pwr"/>
<pin name="SDATA_IN"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SYNC" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="SENSE_A" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="PORT-B_L" direction="in"/>
<pin name="PORT-B_R" direction="in"/>
<pin name="PORT-C_L" direction="in"/>
<pin name="PORT-C_R" direction="in"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VREF_FILT" direction="out"/>
<pin name="MIC_BIAS-B" direction="out"/>
<pin name="MIC_BIAS-C" direction="out"/>
<pin name="SENSE_SRC" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="PORT-D_L" direction="out"/>
<pin name="PORT-D_R" direction="out"/>
<pin name="MONO_OUT" direction="out"/>
<pin name="AVDD@1" direction="in"/>
<pin name="PORT-A_L" direction="out"/>
<pin name="PORT-A_R" direction="out"/>
<pin name="AVSS@1" direction="pwr"/>
<pin name="GPIO_0/JS_1"/>
<pin name="GPIO_1/JS_0"/>
<pin name="S/PDIF_OUT" direction="out"/>
</symbol>
<symbol name="AD1985">
<pin name="DVDD1" direction="in"/>
<pin name="XTL_IN" direction="in"/>
<pin name="XTL_OUT" direction="out"/>
<pin name="DVSS1" direction="in"/>
<pin name="SDATA_OUT" direction="in"/>
<pin name="DVSS2" direction="in"/>
<pin name="SDATA_IN" direction="out"/>
<pin name="DVDD2" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="JS3" direction="in"/>
<pin name="PHONE_IN" direction="in"/>
<pin name="AUX_L" direction="in"/>
<pin name="AUX_R" direction="in"/>
<pin name="JS1" direction="in"/>
<pin name="JS0" direction="in"/>
<pin name="CD_L" direction="in"/>
<pin name="CD_GND_REF" direction="in"/>
<pin name="CD_R" direction="in"/>
<pin name="MIC1" direction="in"/>
<pin name="MIC2" direction="in"/>
<pin name="LINE_IN_L" direction="in"/>
<pin name="LINE_IN_R" direction="in"/>
<pin name="AVDD1" direction="in"/>
<pin name="AVSS1" direction="in"/>
<pin name="VREF" direction="out"/>
<pin name="VREFOUT" direction="out"/>
<pin name="AFILT1" direction="out"/>
<pin name="AFLIT2" direction="out"/>
<pin name="CENTER_OUT"/>
<pin name="LFE_OUT"/>
<pin name="JS2" direction="in"/>
<pin name="AVDD4" direction="in"/>
<pin name="LINE_OUT_L/SURR_L" direction="out"/>
<pin name="LINE_OUT_R/SURR_R" direction="out"/>
<pin name="MONO_OUT" direction="out"/>
<pin name="AVDD2" direction="in"/>
<pin name="SURR_OUT_L/HP_OUT_L" direction="out"/>
<pin name="AVSS2" direction="in"/>
<pin name="SURR_OUT_R/HP_OUT_R" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="AVDD3" direction="in"/>
<pin name="AVSS3" direction="in"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="EAPD" direction="out"/>
<pin name="SPDIF" direction="out"/>
<pin name="BIT_CLK" direction="in"/>
</symbol>
<symbol name="AD210">
<pin name="VO" direction="out"/>
<pin name="OCOM" direction="out"/>
<pin name="+VOSS" direction="out"/>
<pin name="-VOSS" direction="out"/>
<pin name="+VISS" direction="in"/>
<pin name="-VISS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="ICOM" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="PWR_COM" direction="in"/>
<pin name="PWR" direction="in"/>
</symbol>
<symbol name="AD215">
<pin name="OUTHI" direction="out"/>
<pin name="TRIM" direction="pas"/>
<pin name="+15V" direction="in"/>
<pin name="-15V" direction="in"/>
<pin name="+VISO" direction="out"/>
<pin name="-VISO" direction="out"/>
<pin name="FB" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="INCOM" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="PWRRTN" direction="in"/>
<pin name="OUTLO" direction="out"/>
</symbol>
<symbol name="AD526">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!CLK" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B" direction="in"/>
<pin name="VS+" direction="in"/>
<pin name="VO/F" direction="in"/>
<pin name="VO/S" direction="in"/>
<pin name="VS-" direction="in"/>
<pin name="AGND1" direction="in"/>
<pin name="AGND2" direction="in"/>
<pin name="NULL@2" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="NULL@1" direction="in"/>
<pin name="DGND" direction="in"/>
</symbol>
<symbol name="AD625">
<pin name="-IN" direction="in"/>
<pin name="-GAINSENSE" direction="in"/>
<pin name="-GAINDRIVE" direction="in"/>
<pin name="+GAINDRIVE" direction="in"/>
<pin name="+GAINSENSE" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="+VS" direction="in"/>
<pin name="-VS" direction="in"/>
<pin name="RTINULL@1" direction="pas"/>
<pin name="RTINULL@2" direction="pas"/>
<pin name="RTONULL@1" direction="pas"/>
<pin name="RTONULL@2" direction="pas"/>
</symbol>
<symbol name="OP_OFFSET+-VS">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="-VS" direction="in"/>
<pin name="+VS" direction="in"/>
<pin name="OFF@1" direction="pas"/>
<pin name="OFF@2" direction="pas"/>
</symbol>
<symbol name="OP-COMP+-VS">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="-VS" direction="in"/>
<pin name="+VS" direction="in"/>
<pin name="OFF@1" direction="pas"/>
<pin name="OFF@2" direction="pas"/>
<pin name="COMP" direction="pas"/>
</symbol>
<symbol name="AD7676">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="AGND@1" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="REFGND" direction="in"/>
<pin name="DVDD" direction="in"/>
<pin name="DGND@1" direction="in"/>
<pin name="OVDD" direction="in"/>
<pin name="OGND" direction="in"/>
<pin name="SER/!PAR" direction="in"/>
<pin name="BUSY" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="DIVSCLK0/D2"/>
<pin name="DIVSCLK1/D3"/>
<pin name="EXT/!INT!/D4"/>
<pin name="INVSYNC/D5"/>
<pin name="INVSCLK/D6"/>
<pin name="RDC/SDIN/D7"/>
<pin name="SDOUT/D8" direction="out"/>
<pin name="SCLK/D9"/>
<pin name="SYNC/D10" direction="out"/>
<pin name="RDERROR/D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13" direction="out"/>
<pin name="D14" direction="out"/>
<pin name="D15" direction="out"/>
<pin name="!CS" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="OB/!2C" direction="in"/>
<pin name="!CNVST" direction="in"/>
<pin name="BYTESWAP" direction="in"/>
<pin name="AGND@2" direction="in"/>
<pin name="DGND@2" direction="in"/>
</symbol>
<symbol name="AD7730">
<pin name="VBIAS" direction="pas"/>
<pin name="AIN1+" direction="in"/>
<pin name="AIN1-" direction="in"/>
<pin name="AIN2+/D1"/>
<pin name="AIN2-/D0"/>
<pin name="ACX" direction="out"/>
<pin name="!ACX" direction="out"/>
<pin name="AGND" direction="in"/>
<pin name="DGND" direction="in"/>
<pin name="POL" direction="in"/>
<pin name="!RDY" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="MCLKIN" direction="in"/>
<pin name="MCLKOUT" direction="out"/>
<pin name="!SYNC" direction="in"/>
<pin name="!STANDBY" direction="in"/>
<pin name="REFIN-" direction="in"/>
<pin name="REFIN+" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="DVDD" direction="in"/>
</symbol>
<symbol name="AD8015">
<pin name="IN" direction="in"/>
<pin name="VBYP" direction="in"/>
<pin name="-VS" direction="in"/>
<pin name="+VS" direction="in"/>
<pin name="+OUT" direction="out"/>
<pin name="-OUT" direction="out"/>
</symbol>
<symbol name="OP+-VSDISABLE">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="-VS" direction="in"/>
<pin name="+VS" direction="in"/>
<pin name="DISABLE" direction="pas"/>
</symbol>
<symbol name="AD8074">
<pin name="!OE" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="OUT0" direction="hiz"/>
<pin name="OUT1" direction="hiz"/>
<pin name="OUT2" direction="hiz"/>
<pin name="VEE@1" direction="in"/>
<pin name="VEE@2" direction="in"/>
<pin name="VCC@1" direction="in"/>
<pin name="VCC@2" direction="in"/>
<pin name="AGND@1" direction="in"/>
<pin name="AGND@2" direction="in"/>
<pin name="VEE@3" direction="in"/>
<pin name="VCC@3" direction="in"/>
<pin name="DGND" direction="in"/>
</symbol>
<symbol name="OP-GAIN">
<pin name="IN+" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="OP_PD">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!POWERDOWN" direction="pas"/>
</symbol>
<symbol name="PWR+-2">
<pin name="V+@1" direction="pwr"/>
<pin name="V-@1" direction="pwr"/>
<pin name="V+@2" direction="pwr"/>
<pin name="V-@2" direction="pwr"/>
</symbol>
<symbol name="ADAU1592">
<pin name="AINL" direction="in"/>
<pin name="AINR" direction="in"/>
<pin name="SLC_TH" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="DVDD" direction="in"/>
<pin name="DGND" direction="in"/>
<pin name="PVDD@1" direction="in"/>
<pin name="PVDD@2" direction="in"/>
<pin name="PVDD@3" direction="in"/>
<pin name="PVDD@4" direction="in"/>
<pin name="PGND@1" direction="in"/>
<pin name="PGND@2" direction="in"/>
<pin name="PGND@3" direction="in"/>
<pin name="PGND@4" direction="in"/>
<pin name="OUTL+@1" direction="pas"/>
<pin name="OUTL-@1" direction="pas"/>
<pin name="OUTR+@1" direction="pas"/>
<pin name="OUTR-@1" direction="pas"/>
<pin name="XTI" direction="in"/>
<pin name="XTO" direction="out"/>
<pin name="MO/!ST" direction="in"/>
<pin name="!STDN" direction="in"/>
<pin name="!MUTE" direction="in"/>
<pin name="!ERR" direction="out"/>
<pin name="!OTW" direction="out"/>
<pin name="PGA0" direction="in"/>
<pin name="PGA1" direction="in"/>
<pin name="OUTL+@2" direction="out"/>
<pin name="OUTL+@3" direction="pas"/>
<pin name="OUTL-@2" direction="out"/>
<pin name="OUTL-@3" direction="pas"/>
<pin name="OUTR+@2" direction="out"/>
<pin name="OUTR+@3" direction="pas"/>
<pin name="OUTR-@2" direction="out"/>
<pin name="OUTR-@3" direction="pas"/>
<pin name="TEST0" direction="in"/>
<pin name="TEST1" direction="in"/>
<pin name="TEST3" direction="in"/>
<pin name="TEST8" direction="in"/>
<pin name="TEST9" direction="in"/>
<pin name="TEST12" direction="in"/>
<pin name="TEST13" direction="in"/>
<pin name="PVDD@5" direction="in"/>
<pin name="PVDD@6" direction="in"/>
<pin name="PVDD@7" direction="in"/>
<pin name="PVDD@8" direction="in"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="ADAV801">
<pin name="VINR" direction="in"/>
<pin name="VINL" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DIR_LF" direction="in"/>
<pin name="DIR_GND" direction="in"/>
<pin name="DIR_VDD" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLATCH" direction="in"/>
<pin name="CIN" direction="in"/>
<pin name="CCLK" direction="in"/>
<pin name="COUT" direction="out"/>
<pin name="ZEROL/INT" direction="out"/>
<pin name="ZEROR" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="ILRCLK"/>
<pin name="IBCLK"/>
<pin name="ISDATA" direction="in"/>
<pin name="OLRCLK"/>
<pin name="OBCLK"/>
<pin name="OSDATA" direction="out"/>
<pin name="DIRIN" direction="in"/>
<pin name="ODVDD" direction="in"/>
<pin name="ODGND" direction="in"/>
<pin name="DITOUT" direction="out"/>
<pin name="OAUXLRCLK"/>
<pin name="OAUXBCLK"/>
<pin name="OAUXSDATA" direction="out"/>
<pin name="IAUXLRCLK"/>
<pin name="IAUXBCLK"/>
<pin name="IAUXSDATA" direction="in"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="MCLKI" direction="in"/>
<pin name="MCLKO" direction="out"/>
<pin name="XOUT" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="SYSCLK3" direction="out"/>
<pin name="SYSCLK2" direction="out"/>
<pin name="SYSCLK1" direction="out"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="PLL_VDD" direction="in"/>
<pin name="PLL_GND" direction="in"/>
<pin name="PLL_LF1" direction="in"/>
<pin name="PLL_LF2" direction="in"/>
<pin name="ADGND" direction="pwr"/>
<pin name="ADVDD" direction="pwr"/>
<pin name="VOUTR" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="VOUTL" direction="out"/>
<pin name="NC@1" direction="nc"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="FILTD" direction="in"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="CAPRN" direction="in"/>
<pin name="CAPRP" direction="in"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="CAPLP" direction="in"/>
<pin name="CAPLN" direction="in"/>
</symbol>
<symbol name="ADAV803">
<pin name="VINR" direction="in"/>
<pin name="VINL" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DIR_LF" direction="in"/>
<pin name="DIR_GND" direction="in"/>
<pin name="DIR_VDD" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="AD0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="ZEROL/INT" direction="out"/>
<pin name="ZEROR" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="ILRCLK"/>
<pin name="IBCLK"/>
<pin name="ISDATA" direction="in"/>
<pin name="OLRCLK"/>
<pin name="OBCLK"/>
<pin name="OSDATA" direction="out"/>
<pin name="DIRIN" direction="in"/>
<pin name="ODVDD" direction="pwr"/>
<pin name="ODGND" direction="pwr"/>
<pin name="DITOUT" direction="out"/>
<pin name="OAUXLRCLK"/>
<pin name="OAUXBCLK"/>
<pin name="OAUXSDATA" direction="out"/>
<pin name="IAUXLRCLK"/>
<pin name="IAUXBCLK"/>
<pin name="IAUXSDATA" direction="in"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="MCLKI" direction="in"/>
<pin name="MCLKO" direction="out"/>
<pin name="XOUT" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="SYSCLK3" direction="out"/>
<pin name="SYSCLK2" direction="out"/>
<pin name="SYSCLK1" direction="out"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="PLL_VDD" direction="in"/>
<pin name="PLL_GND" direction="in"/>
<pin name="PLL_LF1" direction="in"/>
<pin name="PLL_LF2" direction="in"/>
<pin name="ADGND" direction="pwr"/>
<pin name="ADVDD" direction="pwr"/>
<pin name="VOUTR" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="VOUTL" direction="out"/>
<pin name="NC@1" direction="nc"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="FILTD" direction="in"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="CAPRN" direction="in"/>
<pin name="CAPRP" direction="in"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="CAPLP" direction="in"/>
<pin name="CAPLN" direction="in"/>
</symbol>
<symbol name="ADAV804">
<pin name="VINR" direction="in"/>
<pin name="VINL" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="DIR_LF" direction="in"/>
<pin name="DIR_GND" direction="in"/>
<pin name="DIR_VDD" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="AD0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="ZEROL/INT" direction="out"/>
<pin name="ZEROR" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="ILRCLK"/>
<pin name="IBCLK"/>
<pin name="ISDATA" direction="in"/>
<pin name="OLRCLK"/>
<pin name="OBCLK"/>
<pin name="OSDATA" direction="out"/>
<pin name="DIRIN" direction="in"/>
<pin name="ODVDD" direction="pwr"/>
<pin name="ODGND" direction="pwr"/>
<pin name="DITOUT" direction="out"/>
<pin name="OAUXLRCLK"/>
<pin name="OAUXBCLK"/>
<pin name="OAUXSDATA" direction="out"/>
<pin name="IAUXLRCLK"/>
<pin name="IAUXBCLK"/>
<pin name="IAUXSDATA" direction="in"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="MCLKI" direction="in"/>
<pin name="MCLKO" direction="out"/>
<pin name="XOUT" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="SYSCLK3" direction="out"/>
<pin name="SYSCLK2" direction="out"/>
<pin name="SYSCLK1" direction="out"/>
<pin name="DGND@2" direction="in"/>
<pin name="PLL_VDD" direction="in"/>
<pin name="PLL_GND" direction="in"/>
<pin name="PLL_LF1" direction="in"/>
<pin name="PLL_LF2" direction="in"/>
<pin name="ADGND" direction="pwr"/>
<pin name="ADVDD" direction="pwr"/>
<pin name="VOUTR" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="OUTPUT" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="FILTD" direction="in"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AVDD@2" direction="in"/>
<pin name="CAPRN" direction="in"/>
<pin name="CAPRP" direction="in"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="CAPLP" direction="in"/>
<pin name="CAPLN" direction="in"/>
</symbol>
<symbol name="ADG-SWITCH-CLOSE-INV">
<pin name="IN" direction="in"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="ADG-SWITCH-OPEN-INV">
<pin name="IN" direction="in"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="ADG-SWITCH-OPEN">
<pin name="IN" direction="in"/>
<pin name="S" direction="pas"/>
<pin name="D" direction="pas"/>
</symbol>
<symbol name="PWR-VSS-VDD-GND-VL">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VL" direction="pwr"/>
</symbol>
<symbol name="ADSP_21368">
<pin name="ACK" direction="in"/>
<pin name="ADDR0" direction="out"/>
<pin name="ADDR1" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="ADDR20" direction="out"/>
<pin name="ADDR21" direction="out"/>
<pin name="ADDR22" direction="out"/>
<pin name="ADDR23" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="BOOTCFG0" direction="in"/>
<pin name="BOOTCFG1" direction="in"/>
<pin name="BR1_B"/>
<pin name="BR2_B"/>
<pin name="BR3_B"/>
<pin name="BR4_B"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="CLK_CFG0" direction="in"/>
<pin name="CLK_CFG1" direction="in"/>
<pin name="DAI1"/>
<pin name="DAI2"/>
<pin name="DAI3"/>
<pin name="DAI4"/>
<pin name="DAI5"/>
<pin name="DAI6"/>
<pin name="DAI7"/>
<pin name="DAI8"/>
<pin name="DAI9"/>
<pin name="DAI10"/>
<pin name="DAI11"/>
<pin name="DAI12"/>
<pin name="DAI13"/>
<pin name="DAI14"/>
<pin name="DAI15"/>
<pin name="DAI16"/>
<pin name="DAI17"/>
<pin name="DAI18"/>
<pin name="DAI19"/>
<pin name="DAI20"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="DATA16"/>
<pin name="DATA17"/>
<pin name="DATA18"/>
<pin name="DATA19"/>
<pin name="DATA20"/>
<pin name="DATA21"/>
<pin name="DATA22"/>
<pin name="DATA23"/>
<pin name="DATA24"/>
<pin name="DATA25"/>
<pin name="DATA26"/>
<pin name="DATA27"/>
<pin name="DATA28"/>
<pin name="DATA29"/>
<pin name="DATA30"/>
<pin name="DATA31"/>
<pin name="DPI1"/>
<pin name="DPI2"/>
<pin name="DPI3"/>
<pin name="DPI4"/>
<pin name="DPI5"/>
<pin name="DPI6"/>
<pin name="DPI7"/>
<pin name="DPI8"/>
<pin name="DPI9"/>
<pin name="DPI10"/>
<pin name="DPI11"/>
<pin name="DPI12"/>
<pin name="DPI13"/>
<pin name="DPI14"/>
<pin name="EMU_B" direction="out"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="GND@37" direction="pwr"/>
<pin name="GND@38" direction="pwr"/>
<pin name="GND@39" direction="pwr"/>
<pin name="GND@40" direction="pwr"/>
<pin name="GND@41" direction="pwr"/>
<pin name="GND@42" direction="pwr"/>
<pin name="GND@43" direction="pwr"/>
<pin name="GND@44" direction="pwr"/>
<pin name="GND@45" direction="pwr"/>
<pin name="GND@46" direction="pwr"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@48" direction="pwr"/>
<pin name="GND@49" direction="pwr"/>
<pin name="GND@50" direction="pwr"/>
<pin name="GND@51" direction="pwr"/>
<pin name="GND@52" direction="pwr"/>
<pin name="GND@53" direction="pwr"/>
<pin name="GND@54" direction="pwr"/>
<pin name="GND@55" direction="pwr"/>
<pin name="GND@56" direction="pwr"/>
<pin name="GND@57" direction="pwr"/>
<pin name="ID0" direction="in"/>
<pin name="ID1" direction="in"/>
<pin name="ID2" direction="in"/>
<pin name="IOVDD@0" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="IOVDD@2" direction="pwr"/>
<pin name="IOVDD@3" direction="pwr"/>
<pin name="IOVDD@4" direction="pwr"/>
<pin name="IOVDD@5" direction="pwr"/>
<pin name="IOVDD@6" direction="pwr"/>
<pin name="IOVDD@7" direction="pwr"/>
<pin name="IOVDD@8" direction="pwr"/>
<pin name="IOVDD@9" direction="pwr"/>
<pin name="IOVDD@10" direction="pwr"/>
<pin name="IOVDD@11" direction="pwr"/>
<pin name="IOVDD@12" direction="pwr"/>
<pin name="IOVDD@13" direction="pwr"/>
<pin name="IOVDD@14" direction="pwr"/>
<pin name="IOVDD@15" direction="pwr"/>
<pin name="IOVDD@16" direction="pwr"/>
<pin name="IOVDD@17" direction="pwr"/>
<pin name="IOVDD@18" direction="pwr"/>
<pin name="IOVDD@19" direction="pwr"/>
<pin name="IOVDD@20" direction="pwr"/>
<pin name="IOVDD@21" direction="pwr"/>
<pin name="IOVDD@22" direction="pwr"/>
<pin name="MS0_B" direction="out"/>
<pin name="MS1_B" direction="out"/>
<pin name="NC0" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="NC5" direction="pas"/>
<pin name="NC6" direction="pas"/>
<pin name="NC7" direction="pas"/>
<pin name="NC8" direction="pas"/>
<pin name="NC9" direction="pas"/>
<pin name="RD_B" direction="out"/>
<pin name="RESET_B" direction="in"/>
<pin name="RPBA" direction="in"/>
<pin name="SDA10" direction="out"/>
<pin name="SDCAS_B" direction="out"/>
<pin name="SDCKE" direction="out"/>
<pin name="SDCLK0"/>
<pin name="SDCLK1"/>
<pin name="SDRAS_B" direction="out"/>
<pin name="SDWE_B" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="VDD@31" direction="pwr"/>
<pin name="VDD@32" direction="pwr"/>
<pin name="VDD@33" direction="pwr"/>
<pin name="VDD@34" direction="pwr"/>
<pin name="WR_B" direction="out"/>
<pin name="XTAL" direction="out"/>
</symbol>
<symbol name="ADSP_21369">
<pin name="ACK" direction="in"/>
<pin name="ADDR0" direction="out"/>
<pin name="ADDR1" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="ADDR20" direction="out"/>
<pin name="ADDR21" direction="out"/>
<pin name="ADDR22" direction="out"/>
<pin name="ADDR23" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="BOOTCFG0" direction="in"/>
<pin name="BOOTCFG1" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="CLK_CFG0" direction="in"/>
<pin name="CLK_CFG1" direction="in"/>
<pin name="DAI1"/>
<pin name="DAI2"/>
<pin name="DAI3"/>
<pin name="DAI4"/>
<pin name="DAI5"/>
<pin name="DAI6"/>
<pin name="DAI7"/>
<pin name="DAI8"/>
<pin name="DAI9"/>
<pin name="DAI10"/>
<pin name="DAI11"/>
<pin name="DAI12"/>
<pin name="DAI13"/>
<pin name="DAI14"/>
<pin name="DAI15"/>
<pin name="DAI16"/>
<pin name="DAI17"/>
<pin name="DAI18"/>
<pin name="DAI19"/>
<pin name="DAI20"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA6"/>
<pin name="DATA7"/>
<pin name="DATA8"/>
<pin name="DATA9"/>
<pin name="DATA10"/>
<pin name="DATA11"/>
<pin name="DATA12"/>
<pin name="DATA13"/>
<pin name="DATA14"/>
<pin name="DATA15"/>
<pin name="DATA16"/>
<pin name="DATA17"/>
<pin name="DATA18"/>
<pin name="DATA19"/>
<pin name="DATA20"/>
<pin name="DATA21"/>
<pin name="DATA22"/>
<pin name="DATA23"/>
<pin name="DATA24"/>
<pin name="DATA25"/>
<pin name="DATA26"/>
<pin name="DATA27"/>
<pin name="DATA28"/>
<pin name="DATA29"/>
<pin name="DATA30"/>
<pin name="DATA31"/>
<pin name="DPI1"/>
<pin name="DPI2"/>
<pin name="DPI3"/>
<pin name="DPI4"/>
<pin name="DPI5"/>
<pin name="DPI6"/>
<pin name="DPI7"/>
<pin name="DPI8"/>
<pin name="DPI9"/>
<pin name="DPI10"/>
<pin name="DPI11"/>
<pin name="DPI12"/>
<pin name="DPI13"/>
<pin name="DPI14"/>
<pin name="EMU_B" direction="out"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="IOVDD@0" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="IOVDD@2" direction="pwr"/>
<pin name="IOVDD@3" direction="pwr"/>
<pin name="IOVDD@4" direction="pwr"/>
<pin name="IOVDD@5" direction="pwr"/>
<pin name="IOVDD@6" direction="pwr"/>
<pin name="IOVDD@7" direction="pwr"/>
<pin name="IOVDD@8" direction="pwr"/>
<pin name="IOVDD@9" direction="pwr"/>
<pin name="IOVDD@10" direction="pwr"/>
<pin name="IOVDD@11" direction="pwr"/>
<pin name="IOVDD@12" direction="pwr"/>
<pin name="IOVDD@13" direction="pwr"/>
<pin name="IOVDD@14" direction="pwr"/>
<pin name="IOVDD@15" direction="pwr"/>
<pin name="IOVDD@16" direction="pwr"/>
<pin name="IOVDD@17" direction="pwr"/>
<pin name="IOVDD@18" direction="pwr"/>
<pin name="MS0_B" direction="out"/>
<pin name="MS1_B" direction="out"/>
<pin name="RD_B" direction="out"/>
<pin name="RESET_B" direction="in"/>
<pin name="SDA10" direction="out"/>
<pin name="SDCAS_B" direction="out"/>
<pin name="SDCKE" direction="out"/>
<pin name="SDCLK0"/>
<pin name="SDRAS_B" direction="out"/>
<pin name="SDWE_B" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="WR_B" direction="out"/>
<pin name="XTAL" direction="out"/>
</symbol>
<symbol name="ADSP_21375">
<pin name="DATA15"/>
<pin name="DATA14"/>
<pin name="DATA13"/>
<pin name="DATA12"/>
<pin name="DATA11"/>
<pin name="DATA10"/>
<pin name="DATA9"/>
<pin name="DATA8"/>
<pin name="DATA7"/>
<pin name="DATA6"/>
<pin name="DATA4"/>
<pin name="DATA5"/>
<pin name="DATA2"/>
<pin name="DATA3"/>
<pin name="DATA0"/>
<pin name="DATA1"/>
<pin name="ADDR0" direction="out"/>
<pin name="ADDR2" direction="out"/>
<pin name="ADDR1" direction="out"/>
<pin name="ADDR4" direction="out"/>
<pin name="ADDR3" direction="out"/>
<pin name="ADDR5" direction="out"/>
<pin name="ADDR6" direction="out"/>
<pin name="ADDR7" direction="out"/>
<pin name="ADDR8" direction="out"/>
<pin name="ADDR9" direction="out"/>
<pin name="ADDR10" direction="out"/>
<pin name="ADDR11" direction="out"/>
<pin name="ADDR12" direction="out"/>
<pin name="ADDR13" direction="out"/>
<pin name="CLKIN" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="ADDR14" direction="out"/>
<pin name="ADDR15" direction="out"/>
<pin name="ADDR16" direction="out"/>
<pin name="ADDR17" direction="out"/>
<pin name="ADDR18" direction="out"/>
<pin name="ADDR19" direction="out"/>
<pin name="ADDR20" direction="out"/>
<pin name="ADDR21" direction="out"/>
<pin name="ADDR23" direction="out"/>
<pin name="ADDR22" direction="out"/>
<pin name="MS1" direction="out"/>
<pin name="MS0" direction="out"/>
<pin name="SDCAS" direction="out"/>
<pin name="SDRAS" direction="out"/>
<pin name="SDCKE" direction="out"/>
<pin name="SDWE" direction="out"/>
<pin name="WR" direction="out"/>
<pin name="SDA10" direction="out"/>
<pin name="SDCLK0" direction="out"/>
<pin name="RD" direction="out"/>
<pin name="ACK" direction="in"/>
<pin name="FLAG3"/>
<pin name="FLAG2"/>
<pin name="FLAG1"/>
<pin name="FLAG0"/>
<pin name="DAI20"/>
<pin name="DAI19"/>
<pin name="DAI18"/>
<pin name="DAI17"/>
<pin name="DAI16"/>
<pin name="DAI15"/>
<pin name="DAI14"/>
<pin name="DAI13"/>
<pin name="DAI12"/>
<pin name="DAI11"/>
<pin name="DAI10"/>
<pin name="DAI8"/>
<pin name="DAI9"/>
<pin name="DAI6"/>
<pin name="DAI7"/>
<pin name="DAI5"/>
<pin name="TDI" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="CLK_CFG0" direction="in"/>
<pin name="BOOTCFG0" direction="in"/>
<pin name="CLK_CFG1" direction="in"/>
<pin name="EMU" direction="out"/>
<pin name="BOOTCFG1" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DAI4"/>
<pin name="DAI2"/>
<pin name="DAI3"/>
<pin name="DAI1"/>
<pin name="DPI14"/>
<pin name="DPI13"/>
<pin name="DPI12"/>
<pin name="DPI11"/>
<pin name="DPI10"/>
<pin name="DPI9"/>
<pin name="DPI8"/>
<pin name="DPI7"/>
<pin name="DPI6"/>
<pin name="DPI5"/>
<pin name="DPI4"/>
<pin name="DPI3"/>
<pin name="DPI1"/>
<pin name="DPI2"/>
<pin name="CLKOUT"/>
<pin name="RESET" direction="in"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="NC0" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="NC5" direction="pas"/>
<pin name="NC6" direction="pas"/>
<pin name="NC7" direction="pas"/>
<pin name="NC8" direction="pas"/>
<pin name="NC9" direction="pas"/>
<pin name="NC10" direction="pas"/>
<pin name="NC11" direction="pas"/>
<pin name="NC12" direction="pas"/>
<pin name="NC13" direction="pas"/>
<pin name="NC14" direction="pas"/>
<pin name="NC15" direction="pas"/>
<pin name="NC16" direction="pas"/>
<pin name="NC17" direction="pas"/>
<pin name="NC18" direction="pas"/>
<pin name="NC19" direction="pas"/>
<pin name="NC20" direction="pas"/>
<pin name="NC21" direction="pas"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="IOVDD@0" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="IOVDD@2" direction="pwr"/>
<pin name="IOVDD@3" direction="pwr"/>
<pin name="IOVDD@4" direction="pwr"/>
<pin name="IOVDD@5" direction="pwr"/>
<pin name="IOVDD@6" direction="pwr"/>
<pin name="IOVDD@7" direction="pwr"/>
<pin name="IOVDD@8" direction="pwr"/>
<pin name="IOVDD@9" direction="pwr"/>
<pin name="IOVDD@10" direction="pwr"/>
<pin name="IOVDD@11" direction="pwr"/>
<pin name="IOVDD@12" direction="pwr"/>
<pin name="IOVDD@13" direction="pwr"/>
<pin name="IOVDD@14" direction="pwr"/>
<pin name="IOVDD@15" direction="pwr"/>
<pin name="IOVDD@16" direction="pwr"/>
<pin name="IOVDD@17" direction="pwr"/>
</symbol>
<symbol name="ADSP_21462W">
<pin name="AMI_ACK" direction="in"/>
<pin name="AMI_ADDR0"/>
<pin name="AMI_ADDR01"/>
<pin name="AMI_ADDR02"/>
<pin name="AMI_ADDR03"/>
<pin name="AMI_ADDR04"/>
<pin name="AMI_ADDR05"/>
<pin name="AMI_ADDR06"/>
<pin name="AMI_ADDR07"/>
<pin name="AMI_ADDR08"/>
<pin name="AMI_ADDR09"/>
<pin name="AMI_ADDR10"/>
<pin name="AMI_ADDR11"/>
<pin name="AMI_ADDR12"/>
<pin name="AMI_ADDR13"/>
<pin name="AMI_ADDR14"/>
<pin name="AMI_ADDR15"/>
<pin name="AMI_ADDR16"/>
<pin name="AMI_ADDR17"/>
<pin name="AMI_ADDR18"/>
<pin name="AMI_ADDR19"/>
<pin name="AMI_ADDR20"/>
<pin name="AMI_ADDR21"/>
<pin name="AMI_ADDR22"/>
<pin name="AMI_ADDR23"/>
<pin name="AMI_DATA0"/>
<pin name="AMI_DATA1"/>
<pin name="AMI_DATA2"/>
<pin name="AMI_DATA3"/>
<pin name="AMI_DATA4"/>
<pin name="AMI_DATA5"/>
<pin name="AMI_DATA6"/>
<pin name="AMI_DATA7"/>
<pin name="AMI_MS0_B" direction="out"/>
<pin name="AMI_MS1_B" direction="out"/>
<pin name="AMI_RD_B" direction="out"/>
<pin name="AMI_WR_B" direction="out"/>
<pin name="BOOT_CFG0" direction="in"/>
<pin name="BOOT_CFG1" direction="in"/>
<pin name="BOOT_CFG2" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLKOUT"/>
<pin name="CLK_CFG0" direction="in"/>
<pin name="CLK_CFG1" direction="in"/>
<pin name="DAI_P01"/>
<pin name="DAI_P02"/>
<pin name="DAI_P03"/>
<pin name="DAI_P04"/>
<pin name="DAI_P05"/>
<pin name="DAI_P06"/>
<pin name="DAI_P07"/>
<pin name="DAI_P08"/>
<pin name="DAI_P09"/>
<pin name="DAI_P10"/>
<pin name="DAI_P11"/>
<pin name="DAI_P12"/>
<pin name="DAI_P13"/>
<pin name="DAI_P14"/>
<pin name="DAI_P15"/>
<pin name="DAI_P16"/>
<pin name="DAI_P17"/>
<pin name="DAI_P18"/>
<pin name="DAI_P19"/>
<pin name="DAI_P20"/>
<pin name="DDR2_ADDR0" direction="out"/>
<pin name="DDR2_ADDR01" direction="out"/>
<pin name="DDR2_ADDR02" direction="out"/>
<pin name="DDR2_ADDR03" direction="out"/>
<pin name="DDR2_ADDR04" direction="out"/>
<pin name="DDR2_ADDR05" direction="out"/>
<pin name="DDR2_ADDR06" direction="out"/>
<pin name="DDR2_ADDR07" direction="out"/>
<pin name="DDR2_ADDR08" direction="out"/>
<pin name="DDR2_ADDR09" direction="out"/>
<pin name="DDR2_ADDR10" direction="out"/>
<pin name="DDR2_ADDR11" direction="out"/>
<pin name="DDR2_ADDR12" direction="out"/>
<pin name="DDR2_ADDR13" direction="out"/>
<pin name="DDR2_ADDR14" direction="out"/>
<pin name="DDR2_ADDR15" direction="out"/>
<pin name="DDR2_BA0" direction="out"/>
<pin name="DDR2_BA1" direction="out"/>
<pin name="DDR2_BA2" direction="out"/>
<pin name="DDR2_CAS_B" direction="out"/>
<pin name="DDR2_CKE" direction="out"/>
<pin name="DDR2_CLK0_B" direction="out"/>
<pin name="DDR2_CLK0" direction="out"/>
<pin name="DDR2_CLK1_B" direction="out"/>
<pin name="DDR2_CLK1" direction="out"/>
<pin name="DDR2_CS0_B" direction="out"/>
<pin name="DDR2_CS1_B" direction="out"/>
<pin name="DDR2_CS2_B" direction="out"/>
<pin name="DDR2_CS3_B" direction="out"/>
<pin name="DDR2_DATA0"/>
<pin name="DDR2_DATA01"/>
<pin name="DDR2_DATA02"/>
<pin name="DDR2_DATA03"/>
<pin name="DDR2_DATA04"/>
<pin name="DDR2_DATA05"/>
<pin name="DDR2_DATA06"/>
<pin name="DDR2_DATA07"/>
<pin name="DDR2_DATA08"/>
<pin name="DDR2_DATA09"/>
<pin name="DDR2_DATA10"/>
<pin name="DDR2_DATA11"/>
<pin name="DDR2_DATA12"/>
<pin name="DDR2_DATA13"/>
<pin name="DDR2_DATA14"/>
<pin name="DDR2_DATA15"/>
<pin name="DDR2_DM0" direction="out"/>
<pin name="DDR2_DM1" direction="out"/>
<pin name="DDR2_DQS0"/>
<pin name="DDR2_DQS0_B"/>
<pin name="DDR2_DQS1"/>
<pin name="DDR2_DQS1_B"/>
<pin name="DDR2_ODT" direction="out"/>
<pin name="DDR2_RAS_B" direction="out"/>
<pin name="DDR2_WE_B" direction="out"/>
<pin name="DPI_P01"/>
<pin name="DPI_P02"/>
<pin name="DPI_P03"/>
<pin name="DPI_P04"/>
<pin name="DPI_P05"/>
<pin name="DPI_P06"/>
<pin name="DPI_P07"/>
<pin name="DPI_P08"/>
<pin name="DPI_P09"/>
<pin name="DPI_P10"/>
<pin name="DPI_P11"/>
<pin name="DPI_P12"/>
<pin name="DPI_P13"/>
<pin name="DPI_P14"/>
<pin name="EMU_B" direction="out"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="LACK_0"/>
<pin name="LACK_1"/>
<pin name="LCLK_0"/>
<pin name="LCLK_1"/>
<pin name="LDAT0_0"/>
<pin name="LDAT0_1"/>
<pin name="LDAT0_2"/>
<pin name="LDAT0_3"/>
<pin name="LDAT0_4"/>
<pin name="LDAT0_5"/>
<pin name="LDAT0_6"/>
<pin name="LDAT0_7"/>
<pin name="LDAT1_0"/>
<pin name="LDAT1_1"/>
<pin name="LDAT1_2"/>
<pin name="LDAT1_3"/>
<pin name="LDAT1_4"/>
<pin name="LDAT1_5"/>
<pin name="LDAT1_6"/>
<pin name="LDAT1_7"/>
<pin name="MLBCLK" direction="in"/>
<pin name="MLBDAT"/>
<pin name="MLBDO"/>
<pin name="MLBSIG"/>
<pin name="MLBSO"/>
<pin name="RESET_B" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="THD_M" direction="pas"/>
<pin name="THD_P" direction="pas"/>
<pin name="TMS" direction="in"/>
<pin name="TRST_B" direction="in"/>
<pin name="XTAL" direction="out"/>
<pin name="VDD_A" direction="pwr"/>
<pin name="VDD_THD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VDD_DDR2@0" direction="pwr"/>
<pin name="VDD_DDR2@1" direction="pwr"/>
<pin name="VDD_DDR2@2" direction="pwr"/>
<pin name="VDD_DDR2@3" direction="pwr"/>
<pin name="VDD_DDR2@4" direction="pwr"/>
<pin name="VDD_DDR2@5" direction="pwr"/>
<pin name="VDD_DDR2@6" direction="pwr"/>
<pin name="VDD_DDR2@7" direction="pwr"/>
<pin name="VDD_DDR2@8" direction="pwr"/>
<pin name="VDD_DDR2@9" direction="pwr"/>
<pin name="VDD_DDR2@10" direction="pwr"/>
<pin name="VDD_DDR2@11" direction="pwr"/>
<pin name="VDD_DDR2@12" direction="pwr"/>
<pin name="VDD_DDR2@13" direction="pwr"/>
<pin name="VDD_DDR2@14" direction="pwr"/>
<pin name="VDD_DDR2@15" direction="pwr"/>
<pin name="VDD_DDR2@16" direction="pwr"/>
<pin name="VDD_EXT@0" direction="pwr"/>
<pin name="VDD_EXT@1" direction="pwr"/>
<pin name="VDD_EXT@2" direction="pwr"/>
<pin name="VDD_EXT@3" direction="pwr"/>
<pin name="VDD_EXT@4" direction="pwr"/>
<pin name="VDD_EXT@5" direction="pwr"/>
<pin name="VDD_EXT@6" direction="pwr"/>
<pin name="VDD_EXT@7" direction="pwr"/>
<pin name="VDD_EXT@8" direction="pwr"/>
<pin name="VDD_EXT@9" direction="pwr"/>
<pin name="VDD_EXT@10" direction="pwr"/>
<pin name="VDD_EXT@11" direction="pwr"/>
<pin name="VDD_EXT@12" direction="pwr"/>
<pin name="VDD_EXT@13" direction="pwr"/>
<pin name="VDD_EXT@14" direction="pwr"/>
<pin name="VDD_EXT@15" direction="pwr"/>
<pin name="VDD_EXT@16" direction="pwr"/>
<pin name="VDD_EXT@17" direction="pwr"/>
<pin name="VDD_EXT@18" direction="pwr"/>
<pin name="VDD_EXT@19" direction="pwr"/>
<pin name="VDD_EXT@20" direction="pwr"/>
<pin name="VDD_INT@0" direction="pwr"/>
<pin name="VDD_INT@1" direction="pwr"/>
<pin name="VDD_INT@2" direction="pwr"/>
<pin name="VDD_INT@3" direction="pwr"/>
<pin name="VDD_INT@4" direction="pwr"/>
<pin name="VDD_INT@5" direction="pwr"/>
<pin name="VDD_INT@6" direction="pwr"/>
<pin name="VDD_INT@7" direction="pwr"/>
<pin name="VDD_INT@8" direction="pwr"/>
<pin name="VDD_INT@9" direction="pwr"/>
<pin name="VDD_INT@10" direction="pwr"/>
<pin name="VDD_INT@11" direction="pwr"/>
<pin name="VDD_INT@12" direction="pwr"/>
<pin name="VDD_INT@13" direction="pwr"/>
<pin name="VDD_INT@14" direction="pwr"/>
<pin name="VDD_INT@15" direction="pwr"/>
<pin name="VDD_INT@16" direction="pwr"/>
<pin name="VDD_INT@17" direction="pwr"/>
<pin name="VDD_INT@18" direction="pwr"/>
<pin name="VDD_INT@19" direction="pwr"/>
<pin name="VDD_INT@20" direction="pwr"/>
<pin name="VDD_INT@21" direction="pwr"/>
<pin name="VDD_INT@22" direction="pwr"/>
<pin name="VDD_INT@23" direction="pwr"/>
<pin name="VDD_INT@24" direction="pwr"/>
<pin name="VDD_INT@25" direction="pwr"/>
<pin name="VDD_INT@26" direction="pwr"/>
<pin name="VDD_INT@27" direction="pwr"/>
<pin name="VDD_INT@28" direction="pwr"/>
<pin name="VDD_INT@29" direction="pwr"/>
<pin name="VDD_INT@30" direction="pwr"/>
<pin name="VDD_INT@31" direction="pwr"/>
<pin name="VDD_INT@32" direction="pwr"/>
<pin name="VREF0" direction="pas"/>
<pin name="VREF1" direction="pas"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="GND@37" direction="pwr"/>
<pin name="GND@38" direction="pwr"/>
<pin name="GND@39" direction="pwr"/>
<pin name="GND@40" direction="pwr"/>
<pin name="GND@41" direction="pwr"/>
<pin name="GND@42" direction="pwr"/>
<pin name="GND@43" direction="pwr"/>
<pin name="GND@44" direction="pwr"/>
<pin name="GND@45" direction="pwr"/>
<pin name="GND@46" direction="pwr"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@48" direction="pwr"/>
<pin name="GND@49" direction="pwr"/>
<pin name="GND@50" direction="pwr"/>
<pin name="GND@51" direction="pwr"/>
<pin name="GND@52" direction="pwr"/>
<pin name="GND@53" direction="pwr"/>
<pin name="GND@54" direction="pwr"/>
<pin name="GND@55" direction="pwr"/>
<pin name="GND@56" direction="pwr"/>
<pin name="GND@57" direction="pwr"/>
<pin name="GND@58" direction="pwr"/>
<pin name="GND@59" direction="pwr"/>
<pin name="GND@60" direction="pwr"/>
<pin name="GND@61" direction="pwr"/>
<pin name="GND@62" direction="pwr"/>
<pin name="GND@63" direction="pwr"/>
<pin name="GND@64" direction="pwr"/>
<pin name="GND@65" direction="pwr"/>
<pin name="GND@66" direction="pwr"/>
<pin name="GND@67" direction="pwr"/>
<pin name="GND@68" direction="pwr"/>
<pin name="GND@69" direction="pwr"/>
<pin name="GND@70" direction="pwr"/>
<pin name="GND@71" direction="pwr"/>
<pin name="GND@72" direction="pwr"/>
<pin name="GND@73" direction="pwr"/>
<pin name="GND@74" direction="pwr"/>
<pin name="GND@75" direction="pwr"/>
<pin name="GND@76" direction="pwr"/>
</symbol>
<symbol name="ADSP_21467">
<pin name="AMI_ACK" direction="in"/>
<pin name="AMI_ADDR0"/>
<pin name="AMI_ADDR01"/>
<pin name="AMI_ADDR02"/>
<pin name="AMI_ADDR03"/>
<pin name="AMI_ADDR04"/>
<pin name="AMI_ADDR05"/>
<pin name="AMI_ADDR06"/>
<pin name="AMI_ADDR07"/>
<pin name="AMI_ADDR08"/>
<pin name="AMI_ADDR09"/>
<pin name="AMI_ADDR10"/>
<pin name="AMI_ADDR11"/>
<pin name="AMI_ADDR12"/>
<pin name="AMI_ADDR13"/>
<pin name="AMI_ADDR14"/>
<pin name="AMI_ADDR15"/>
<pin name="AMI_ADDR16"/>
<pin name="AMI_ADDR17"/>
<pin name="AMI_ADDR18"/>
<pin name="AMI_ADDR19"/>
<pin name="AMI_ADDR20"/>
<pin name="AMI_ADDR21"/>
<pin name="AMI_ADDR22"/>
<pin name="AMI_ADDR23"/>
<pin name="AMI_DATA0"/>
<pin name="AMI_DATA1"/>
<pin name="AMI_DATA2"/>
<pin name="AMI_DATA3"/>
<pin name="AMI_DATA4"/>
<pin name="AMI_DATA5"/>
<pin name="AMI_DATA6"/>
<pin name="AMI_DATA7"/>
<pin name="AMI_MS0_B" direction="out"/>
<pin name="AMI_MS1_B" direction="out"/>
<pin name="AMI_RD_B" direction="out"/>
<pin name="AMI_WR_B" direction="out"/>
<pin name="BOOT_CFG0" direction="in"/>
<pin name="BOOT_CFG1" direction="in"/>
<pin name="BOOT_CFG2" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLKOUT"/>
<pin name="CLK_CFG0" direction="in"/>
<pin name="CLK_CFG1" direction="in"/>
<pin name="DAI_P01"/>
<pin name="DAI_P02"/>
<pin name="DAI_P03"/>
<pin name="DAI_P04"/>
<pin name="DAI_P05"/>
<pin name="DAI_P06"/>
<pin name="DAI_P07"/>
<pin name="DAI_P08"/>
<pin name="DAI_P09"/>
<pin name="DAI_P10"/>
<pin name="DAI_P11"/>
<pin name="DAI_P12"/>
<pin name="DAI_P13"/>
<pin name="DAI_P14"/>
<pin name="DAI_P15"/>
<pin name="DAI_P16"/>
<pin name="DAI_P17"/>
<pin name="DAI_P18"/>
<pin name="DAI_P19"/>
<pin name="DAI_P20"/>
<pin name="DDR2_ADDR0" direction="out"/>
<pin name="DDR2_ADDR01" direction="out"/>
<pin name="DDR2_ADDR02" direction="out"/>
<pin name="DDR2_ADDR03" direction="out"/>
<pin name="DDR2_ADDR04" direction="out"/>
<pin name="DDR2_ADDR05" direction="out"/>
<pin name="DDR2_ADDR06" direction="out"/>
<pin name="DDR2_ADDR07" direction="out"/>
<pin name="DDR2_ADDR08" direction="out"/>
<pin name="DDR2_ADDR09" direction="out"/>
<pin name="DDR2_ADDR10" direction="out"/>
<pin name="DDR2_ADDR11" direction="out"/>
<pin name="DDR2_ADDR12" direction="out"/>
<pin name="DDR2_ADDR13" direction="out"/>
<pin name="DDR2_ADDR14" direction="out"/>
<pin name="DDR2_ADDR15" direction="out"/>
<pin name="DDR2_BA0" direction="out"/>
<pin name="DDR2_BA1" direction="out"/>
<pin name="DDR2_BA2" direction="out"/>
<pin name="DDR2_CAS_B" direction="out"/>
<pin name="DDR2_CKE" direction="out"/>
<pin name="DDR2_CLK0_B" direction="out"/>
<pin name="DDR2_CLK0" direction="out"/>
<pin name="DDR2_CLK1_B" direction="out"/>
<pin name="DDR2_CLK1" direction="out"/>
<pin name="DDR2_CS0_B" direction="out"/>
<pin name="DDR2_CS1_B" direction="out"/>
<pin name="DDR2_CS2_B" direction="out"/>
<pin name="DDR2_CS3_B" direction="out"/>
<pin name="DDR2_DATA0"/>
<pin name="DDR2_DATA01"/>
<pin name="DDR2_DATA02"/>
<pin name="DDR2_DATA03"/>
<pin name="DDR2_DATA04"/>
<pin name="DDR2_DATA05"/>
<pin name="DDR2_DATA06"/>
<pin name="DDR2_DATA07"/>
<pin name="DDR2_DATA08"/>
<pin name="DDR2_DATA09"/>
<pin name="DDR2_DATA10"/>
<pin name="DDR2_DATA11"/>
<pin name="DDR2_DATA12"/>
<pin name="DDR2_DATA13"/>
<pin name="DDR2_DATA14"/>
<pin name="DDR2_DATA15"/>
<pin name="DDR2_DM0" direction="out"/>
<pin name="DDR2_DM1" direction="out"/>
<pin name="DDR2_DQS0"/>
<pin name="DDR2_DQS0_B"/>
<pin name="DDR2_DQS1"/>
<pin name="DDR2_DQS1_B"/>
<pin name="DDR2_ODT" direction="out"/>
<pin name="DDR2_RAS_B" direction="out"/>
<pin name="DDR2_WE_B" direction="out"/>
<pin name="DPI_P01"/>
<pin name="DPI_P02"/>
<pin name="DPI_P03"/>
<pin name="DPI_P04"/>
<pin name="DPI_P05"/>
<pin name="DPI_P06"/>
<pin name="DPI_P07"/>
<pin name="DPI_P08"/>
<pin name="DPI_P09"/>
<pin name="DPI_P10"/>
<pin name="DPI_P11"/>
<pin name="DPI_P12"/>
<pin name="DPI_P13"/>
<pin name="DPI_P14"/>
<pin name="EMU_B" direction="out"/>
<pin name="FLAG0"/>
<pin name="FLAG1"/>
<pin name="FLAG2"/>
<pin name="FLAG3"/>
<pin name="LACK_0"/>
<pin name="LACK_1"/>
<pin name="LCLK_0"/>
<pin name="LCLK_1"/>
<pin name="LDAT0_0"/>
<pin name="LDAT0_1"/>
<pin name="LDAT0_2"/>
<pin name="LDAT0_3"/>
<pin name="LDAT0_4"/>
<pin name="LDAT0_5"/>
<pin name="LDAT0_6"/>
<pin name="LDAT0_7"/>
<pin name="LDAT1_0"/>
<pin name="LDAT1_1"/>
<pin name="LDAT1_2"/>
<pin name="LDAT1_3"/>
<pin name="LDAT1_4"/>
<pin name="LDAT1_5"/>
<pin name="LDAT1_6"/>
<pin name="LDAT1_7"/>
<pin name="RESET_B" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="THD_M" direction="pas"/>
<pin name="THD_P" direction="pas"/>
<pin name="TMS" direction="in"/>
<pin name="TRST_B" direction="in"/>
<pin name="XTAL" direction="out"/>
<pin name="VDD_A" direction="pwr"/>
<pin name="VDD_THD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="NC0" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="VDD_DDR2@0" direction="pwr"/>
<pin name="VDD_DDR2@1" direction="pwr"/>
<pin name="VDD_DDR2@2" direction="pwr"/>
<pin name="VDD_DDR2@3" direction="pwr"/>
<pin name="VDD_DDR2@4" direction="pwr"/>
<pin name="VDD_DDR2@5" direction="pwr"/>
<pin name="VDD_DDR2@6" direction="pwr"/>
<pin name="VDD_DDR2@7" direction="pwr"/>
<pin name="VDD_DDR2@8" direction="pwr"/>
<pin name="VDD_DDR2@9" direction="pwr"/>
<pin name="VDD_DDR2@10" direction="pwr"/>
<pin name="VDD_DDR2@11" direction="pwr"/>
<pin name="VDD_DDR2@12" direction="pwr"/>
<pin name="VDD_DDR2@13" direction="pwr"/>
<pin name="VDD_DDR2@14" direction="pwr"/>
<pin name="VDD_DDR2@15" direction="pwr"/>
<pin name="VDD_DDR2@16" direction="pwr"/>
<pin name="VDD_EXT@0" direction="pwr"/>
<pin name="VDD_EXT@1" direction="pwr"/>
<pin name="VDD_EXT@2" direction="pwr"/>
<pin name="VDD_EXT@3" direction="pwr"/>
<pin name="VDD_EXT@4" direction="pwr"/>
<pin name="VDD_EXT@5" direction="pwr"/>
<pin name="VDD_EXT@6" direction="pwr"/>
<pin name="VDD_EXT@7" direction="pwr"/>
<pin name="VDD_EXT@8" direction="pwr"/>
<pin name="VDD_EXT@9" direction="pwr"/>
<pin name="VDD_EXT@10" direction="pwr"/>
<pin name="VDD_EXT@11" direction="pwr"/>
<pin name="VDD_EXT@12" direction="pwr"/>
<pin name="VDD_EXT@13" direction="pwr"/>
<pin name="VDD_EXT@14" direction="pwr"/>
<pin name="VDD_EXT@15" direction="pwr"/>
<pin name="VDD_EXT@16" direction="pwr"/>
<pin name="VDD_EXT@17" direction="pwr"/>
<pin name="VDD_EXT@18" direction="pwr"/>
<pin name="VDD_EXT@19" direction="pwr"/>
<pin name="VDD_EXT@20" direction="pwr"/>
<pin name="VDD_INT@0" direction="pwr"/>
<pin name="VDD_INT@1" direction="pwr"/>
<pin name="VDD_INT@2" direction="pwr"/>
<pin name="VDD_INT@3" direction="pwr"/>
<pin name="VDD_INT@4" direction="pwr"/>
<pin name="VDD_INT@5" direction="pwr"/>
<pin name="VDD_INT@6" direction="pwr"/>
<pin name="VDD_INT@7" direction="pwr"/>
<pin name="VDD_INT@8" direction="pwr"/>
<pin name="VDD_INT@9" direction="pwr"/>
<pin name="VDD_INT@10" direction="pwr"/>
<pin name="VDD_INT@11" direction="pwr"/>
<pin name="VDD_INT@12" direction="pwr"/>
<pin name="VDD_INT@13" direction="pwr"/>
<pin name="VDD_INT@14" direction="pwr"/>
<pin name="VDD_INT@15" direction="pwr"/>
<pin name="VDD_INT@16" direction="pwr"/>
<pin name="VDD_INT@17" direction="pwr"/>
<pin name="VDD_INT@18" direction="pwr"/>
<pin name="VDD_INT@19" direction="pwr"/>
<pin name="VDD_INT@20" direction="pwr"/>
<pin name="VDD_INT@21" direction="pwr"/>
<pin name="VDD_INT@22" direction="pwr"/>
<pin name="VDD_INT@23" direction="pwr"/>
<pin name="VDD_INT@24" direction="pwr"/>
<pin name="VDD_INT@25" direction="pwr"/>
<pin name="VDD_INT@26" direction="pwr"/>
<pin name="VDD_INT@27" direction="pwr"/>
<pin name="VDD_INT@28" direction="pwr"/>
<pin name="VDD_INT@29" direction="pwr"/>
<pin name="VDD_INT@30" direction="pwr"/>
<pin name="VDD_INT@31" direction="pwr"/>
<pin name="VDD_INT@32" direction="pwr"/>
<pin name="VREF0" direction="pas"/>
<pin name="VREF1" direction="pas"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
<pin name="GND@29" direction="pwr"/>
<pin name="GND@30" direction="pwr"/>
<pin name="GND@31" direction="pwr"/>
<pin name="GND@32" direction="pwr"/>
<pin name="GND@33" direction="pwr"/>
<pin name="GND@34" direction="pwr"/>
<pin name="GND@35" direction="pwr"/>
<pin name="GND@36" direction="pwr"/>
<pin name="GND@37" direction="pwr"/>
<pin name="GND@38" direction="pwr"/>
<pin name="GND@39" direction="pwr"/>
<pin name="GND@40" direction="pwr"/>
<pin name="GND@41" direction="pwr"/>
<pin name="GND@42" direction="pwr"/>
<pin name="GND@43" direction="pwr"/>
<pin name="GND@44" direction="pwr"/>
<pin name="GND@45" direction="pwr"/>
<pin name="GND@46" direction="pwr"/>
<pin name="GND@47" direction="pwr"/>
<pin name="GND@48" direction="pwr"/>
<pin name="GND@49" direction="pwr"/>
<pin name="GND@50" direction="pwr"/>
<pin name="GND@51" direction="pwr"/>
<pin name="GND@52" direction="pwr"/>
<pin name="GND@53" direction="pwr"/>
<pin name="GND@54" direction="pwr"/>
<pin name="GND@55" direction="pwr"/>
<pin name="GND@56" direction="pwr"/>
<pin name="GND@57" direction="pwr"/>
<pin name="GND@58" direction="pwr"/>
<pin name="GND@59" direction="pwr"/>
<pin name="GND@60" direction="pwr"/>
<pin name="GND@61" direction="pwr"/>
<pin name="GND@62" direction="pwr"/>
<pin name="GND@63" direction="pwr"/>
<pin name="GND@64" direction="pwr"/>
<pin name="GND@65" direction="pwr"/>
<pin name="GND@66" direction="pwr"/>
<pin name="GND@67" direction="pwr"/>
<pin name="GND@68" direction="pwr"/>
<pin name="GND@69" direction="pwr"/>
<pin name="GND@70" direction="pwr"/>
<pin name="GND@71" direction="pwr"/>
<pin name="GND@72" direction="pwr"/>
<pin name="GND@73" direction="pwr"/>
<pin name="GND@74" direction="pwr"/>
<pin name="GND@75" direction="pwr"/>
<pin name="GND@76" direction="pwr"/>
</symbol>
<symbol name="ADV7184">
<pin name="VS" direction="out"/>
<pin name="HS" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="DVDDIO" direction="pwr"/>
<pin name="P11" direction="out"/>
<pin name="P10" direction="out"/>
<pin name="P9" direction="out"/>
<pin name="P8" direction="out"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="INT" direction="out"/>
<pin name="SFL" direction="out"/>
<pin name="TEST2" direction="pas"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DVDDIO@1" direction="pwr"/>
<pin name="TEST8" direction="pas"/>
<pin name="TEST12" direction="pas"/>
<pin name="TEST11" direction="pas"/>
<pin name="P7" direction="out"/>
<pin name="P6" direction="out"/>
<pin name="P5" direction="out"/>
<pin name="P4" direction="out"/>
<pin name="P3" direction="out"/>
<pin name="P2" direction="out"/>
<pin name="TEST3" direction="pas"/>
<pin name="LLC2" direction="out"/>
<pin name="LLC1" direction="out"/>
<pin name="XTAL1" direction="out"/>
<pin name="XTAL" direction="in"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="P1" direction="out"/>
<pin name="P0" direction="out"/>
<pin name="TEST10" direction="pas"/>
<pin name="TEST9" direction="pas"/>
<pin name="PWRDN" direction="in"/>
<pin name="ELPF" direction="in"/>
<pin name="PVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="AIN7" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN8" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN9" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="CAPY1" direction="in"/>
<pin name="CAPY2" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="REFOUT" direction="out"/>
<pin name="CML" direction="out"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="CAPC1" direction="in"/>
<pin name="CAPC2" direction="in"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AIN10" direction="in"/>
<pin name="AIN4" direction="in"/>
<pin name="AIN11" direction="in"/>
<pin name="AIN5" direction="in"/>
<pin name="AIN12" direction="in"/>
<pin name="AIN6" direction="in"/>
<pin name="SOY" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="TEST7" direction="pas"/>
<pin name="ALSB" direction="in"/>
<pin name="SDA"/>
<pin name="SCLK" direction="in"/>
<pin name="TEST4" direction="pas"/>
<pin name="TEST0" direction="pas"/>
<pin name="DGND@4" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="P15" direction="out"/>
<pin name="P14" direction="out"/>
<pin name="P13" direction="out"/>
<pin name="P12" direction="out"/>
<pin name="TEST6" direction="pas"/>
<pin name="TEST1" direction="pas"/>
<pin name="OE" direction="in"/>
<pin name="FIELD" direction="out"/>
</symbol>
<symbol name="ADV7194">
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="P8" direction="in"/>
<pin name="P9" direction="in"/>
<pin name="Y0/P10" direction="in"/>
<pin name="Y1/P11" direction="in"/>
<pin name="Y2/P12" direction="in"/>
<pin name="Y3/P13" direction="in"/>
<pin name="Y4/P14" direction="in"/>
<pin name="Y5/P15" direction="in"/>
<pin name="Y6/P16" direction="in"/>
<pin name="Y7/P17" direction="in"/>
<pin name="Y8/P18" direction="in"/>
<pin name="Y9/P19" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="HSYNC"/>
<pin name="VSYNC"/>
<pin name="BLANK"/>
<pin name="CB0" direction="in"/>
<pin name="CB1" direction="in"/>
<pin name="CB2" direction="in"/>
<pin name="CB3" direction="in"/>
<pin name="CB4" direction="in"/>
<pin name="CB5" direction="in"/>
<pin name="TTXREQ" direction="out"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="CLKIN" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="VAA" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="SCRESET/RTC/TR" direction="in"/>
<pin name="ALSB" direction="in"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="RSET2" direction="in"/>
<pin name="COMP2" direction="out"/>
<pin name="DAC_F" direction="out"/>
<pin name="DAC_E" direction="out"/>
<pin name="VAA@1" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="DAC_D" direction="out"/>
<pin name="DAC_C" direction="out"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="VAA@2" direction="pwr"/>
<pin name="DAC_B" direction="out"/>
<pin name="DAC_A" direction="out"/>
<pin name="COMP_1" direction="out"/>
<pin name="VREF"/>
<pin name="RSET1" direction="in"/>
<pin name="PAL_NTSC" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CSO_HSO" direction="out"/>
<pin name="VSO/TTX/CLAMP"/>
<pin name="CR0" direction="in"/>
<pin name="CR1" direction="in"/>
<pin name="CR2" direction="in"/>
<pin name="CR3" direction="in"/>
<pin name="CR4" direction="in"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="CR5" direction="in"/>
<pin name="CR6" direction="in"/>
<pin name="CR7" direction="in"/>
<pin name="CR8" direction="in"/>
<pin name="CR9" direction="in"/>
<pin name="CB6" direction="in"/>
<pin name="CB7" direction="in"/>
<pin name="CB8" direction="in"/>
<pin name="CB9" direction="in"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="DGND@4" direction="pwr"/>
</symbol>
<symbol name="BUF+-OFF">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="-VS" direction="in"/>
<pin name="+VS" direction="in"/>
<pin name="OFF@1" direction="pas"/>
<pin name="OFF@2" direction="pas"/>
</symbol>
<symbol name="NPN+DIODE">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SUB">
<pin name="SUB@1" direction="pas"/>
<pin name="SUB@2" direction="pas"/>
</symbol>
<symbol name="AD8235">
<pin name="REF" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="RG@1" direction="in"/>
<pin name="RG@2" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="SDN" direction="pas"/>
</symbol>
<symbol name="AD5282">
<pin name="!SHDN" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="AD0" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="O1" direction="out"/>
<pin name="A1" direction="pas"/>
<pin name="W1" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="W2" direction="pas"/>
<pin name="B2" direction="pas"/>
</symbol>
<symbol name="AD5280">
<pin name="!SHDN" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VL" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="AD0" direction="in"/>
<pin name="AD1" direction="in"/>
<pin name="O1" direction="out"/>
<pin name="A" direction="pas"/>
<pin name="W" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="O2" direction="out"/>
</symbol>
<symbol name="AD9854">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2/IO_RESET" direction="in"/>
<pin name="A1/SDO" direction="in"/>
<pin name="A0/SDIO" direction="in"/>
<pin name="I/O_UD_CLK" direction="in"/>
<pin name="!WR!/SCLK" direction="in"/>
<pin name="!RD!/!CS!" direction="in"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DGND@4" direction="pwr"/>
<pin name="DGND@5" direction="pwr"/>
<pin name="FSK/BPSK/HOLD" direction="in"/>
<pin name="OSK" direction="in"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="NC@2" direction="nc"/>
<pin name="VOUT" direction="out"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="AVDD@4" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AGND@5" direction="pwr"/>
<pin name="VINP" direction="in"/>
<pin name="VINN" direction="in"/>
<pin name="AVDD@5" direction="pwr"/>
<pin name="AGND@6" direction="pwr"/>
<pin name="AGND@7" direction="pwr"/>
<pin name="AGND@8" direction="pwr"/>
<pin name="IOUT1" direction="out"/>
<pin name="!IOUT1" direction="out"/>
<pin name="!IOUT2" direction="out"/>
<pin name="IOUT2" direction="out"/>
<pin name="AVDD@6" direction="pwr"/>
<pin name="AGND@9" direction="pwr"/>
<pin name="AVDD@7" direction="pwr"/>
<pin name="DACBP" direction="in"/>
<pin name="DACREST" direction="in"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="AGND@10" direction="pwr"/>
<pin name="AVDD@8" direction="pwr"/>
<pin name="PLLFILTER" direction="in"/>
<pin name="AGND@11" direction="pwr"/>
<pin name="NC@5" direction="nc"/>
<pin name="DIFF_CLKENABLE" direction="in"/>
<pin name="AVDD@9" direction="pwr"/>
<pin name="AGND@12" direction="pwr"/>
<pin name="AGND@13" direction="pwr"/>
<pin name="!REFCLK" direction="in"/>
<pin name="REFCLK" direction="in"/>
<pin name="S/P_SELECT" direction="in"/>
<pin name="MASTER_RESET" direction="in"/>
<pin name="DGND@6" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="DVDD@7" direction="pwr"/>
<pin name="DGND@7" direction="pwr"/>
<pin name="DGND@8" direction="pwr"/>
<pin name="DGND@9" direction="pwr"/>
<pin name="DGND@10" direction="pwr"/>
<pin name="DVDD@8" direction="pwr"/>
<pin name="DVDD@9" direction="pwr"/>
</symbol>
<symbol name="AD9912">
<pin name="DVDD_I/O" direction="pwr"/>
<pin name="DVSS@1" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVSS@2" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DVSS@3" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVSS@4" direction="pwr"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="AVDD3@1" direction="pwr"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="AVDD@4" direction="pwr"/>
<pin name="AVDD@5" direction="pwr"/>
<pin name="AVDD@6" direction="pwr"/>
<pin name="SYSCLK" direction="in"/>
<pin name="SYSCLKB" direction="in"/>
<pin name="AVDD@7" direction="pwr"/>
<pin name="AVDD@8" direction="pwr"/>
<pin name="LOOP_FILTER" direction="in"/>
<pin name="CLKMODESEL" direction="in"/>
<pin name="AVSS@1" direction="pwr"/>
<pin name="OUTB" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="AVDD@9" direction="pwr"/>
<pin name="AVDD3@2" direction="pwr"/>
<pin name="OUT_CMOS" direction="out"/>
<pin name="AVSS@2" direction="pwr"/>
<pin name="FDBK_INB" direction="in"/>
<pin name="FDBK_IN" direction="in"/>
<pin name="AVDD@10" direction="pwr"/>
<pin name="AVSS@3" direction="pwr"/>
<pin name="AVDD@11" direction="pwr"/>
<pin name="AVDD@12" direction="pwr"/>
<pin name="AVDD3@3" direction="pwr"/>
<pin name="AVDD3@4" direction="pwr"/>
<pin name="DAC_RSET" direction="in"/>
<pin name="AVDD3@5" direction="pwr"/>
<pin name="DAC_OUT" direction="out"/>
<pin name="DAC_OUTB" direction="out"/>
<pin name="AVSS@4" direction="pwr"/>
<pin name="AVDD@13" direction="pwr"/>
<pin name="S3" direction="in"/>
<pin name="S4" direction="in"/>
<pin name="DVSS@5" direction="pwr"/>
<pin name="DVSS@6" direction="pwr"/>
<pin name="PWRDOWN" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="IO_UPDATE" direction="in"/>
<pin name="CSB" direction="in"/>
<pin name="SDO" direction="in"/>
<pin name="SDIO" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="ADUC845-52">
<pin name="P1_0/AIN1" direction="in"/>
<pin name="P1_1/AIN2" direction="in"/>
<pin name="P1_2/AIN3/REFIN2+" direction="in"/>
<pin name="P1_3/AIN4/REFIN2-" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="REFIN-" direction="in"/>
<pin name="REFIN+" direction="in"/>
<pin name="P1_4/AIN5" direction="in"/>
<pin name="P1_5/AIN6" direction="in"/>
<pin name="P1_6/AIN7/IEXC1"/>
<pin name="P1_7/AIN8/IEXC2"/>
<pin name="AINCOM/DAC"/>
<pin name="DAC" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="P3_0/RXD"/>
<pin name="P3_1/TXD"/>
<pin name="P3_2/INT0"/>
<pin name="P3_3/INT1"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="P3_4/T0"/>
<pin name="P3_5/T1"/>
<pin name="P3_6/WR"/>
<pin name="P3_7/RD"/>
<pin name="SCLK_I2C"/>
<pin name="SDATA"/>
<pin name="P2_0/SCLOCK_SPI"/>
<pin name="P2_1/MOSI"/>
<pin name="P2_2/MISO"/>
<pin name="P2_3/SS/T2"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="P2_4/T2EX"/>
<pin name="P2_5/PWM0"/>
<pin name="P2_6/PWM1"/>
<pin name="P2_7/PWMCLK"/>
<pin name="EA" direction="in"/>
<pin name="PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="P0_0"/>
<pin name="P0_1"/>
<pin name="P0_2"/>
<pin name="P0_3"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="P0_4"/>
<pin name="P0_5"/>
<pin name="P0_6"/>
<pin name="P0_7"/>
</symbol>
<symbol name="ADUC845-56">
<pin name="P1_1/AIN2" direction="in"/>
<pin name="P1_2/AIN3/REFIN2+" direction="in"/>
<pin name="P1_3/AIN4/REFIN2-" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="REFIN-" direction="in"/>
<pin name="REFIN+" direction="in"/>
<pin name="P1_4/AIN5" direction="in"/>
<pin name="P1_5/AIN6" direction="in"/>
<pin name="P1_6/AIN7/IEXC1"/>
<pin name="P1_7/AIN8/IEXC2"/>
<pin name="AINCOM/DAC"/>
<pin name="DAC" direction="out"/>
<pin name="AIN9" direction="in"/>
<pin name="AIN10" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="P3_0/RXD"/>
<pin name="P3_1/TXD"/>
<pin name="P3_2/INT0"/>
<pin name="P3_3/INT1"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="P3_4/T0"/>
<pin name="P3_5/T1"/>
<pin name="P3_6/WR"/>
<pin name="P3_7/RD"/>
<pin name="SCLK_I2C"/>
<pin name="SDATA"/>
<pin name="P2_0/SCLOCK_SPI"/>
<pin name="P2_1/MOSI"/>
<pin name="P2_2/MISO"/>
<pin name="P2_3/SS/T2"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="P2_4/T2EX"/>
<pin name="P2_5/PWM0"/>
<pin name="P2_6/PWM1"/>
<pin name="P2_7/PWMCLK"/>
<pin name="EA" direction="in"/>
<pin name="PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="P0_0"/>
<pin name="P0_1"/>
<pin name="P0_2"/>
<pin name="P0_3"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="P0_4"/>
<pin name="P0_5"/>
<pin name="P0_6"/>
<pin name="P0_7"/>
<pin name="P1_0/AIN1" direction="in"/>
<pin name="EXP" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AD21065L" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SP21065L"/>
<gate name="-GND" symbol="GND37"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="-VCC" symbol="VCC32"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="-GND" pin="GND" pad="3"/>
<connect gate="-GND" pin="GND@1" pad="10"/>
<connect gate="-GND" pin="GND@10" pad="62"/>
<connect gate="-GND" pin="GND@11" pad="68"/>
<connect gate="-GND" pin="GND@12" pad="72"/>
<connect gate="-GND" pin="GND@13" pad="73"/>
<connect gate="-GND" pin="GND@14" pad="81"/>
<connect gate="-GND" pin="GND@15" pad="89"/>
<connect gate="-GND" pin="GND@16" pad="94"/>
<connect gate="-GND" pin="GND@17" pad="99"/>
<connect gate="-GND" pin="GND@18" pad="106"/>
<connect gate="-GND" pin="GND@19" pad="114"/>
<connect gate="-GND" pin="GND@2" pad="14"/>
<connect gate="-GND" pin="GND@20" pad="119"/>
<connect gate="-GND" pin="GND@21" pad="125"/>
<connect gate="-GND" pin="GND@22" pad="129"/>
<connect gate="-GND" pin="GND@23" pad="135"/>
<connect gate="-GND" pin="GND@24" pad="139"/>
<connect gate="-GND" pin="GND@25" pad="150"/>
<connect gate="-GND" pin="GND@26" pad="154"/>
<connect gate="-GND" pin="GND@27" pad="155"/>
<connect gate="-GND" pin="GND@28" pad="159"/>
<connect gate="-GND" pin="GND@29" pad="167"/>
<connect gate="-GND" pin="GND@3" pad="25"/>
<connect gate="-GND" pin="GND@30" pad="168"/>
<connect gate="-GND" pin="GND@31" pad="177"/>
<connect gate="-GND" pin="GND@32" pad="181"/>
<connect gate="-GND" pin="GND@33" pad="186"/>
<connect gate="-GND" pin="GND@34" pad="187"/>
<connect gate="-GND" pin="GND@35" pad="196"/>
<connect gate="-GND" pin="GND@36" pad="204"/>
<connect gate="-GND" pin="GND@4" pad="33"/>
<connect gate="-GND" pin="GND@5" pad="35"/>
<connect gate="-GND" pin="GND@6" pad="41"/>
<connect gate="-GND" pin="GND@7" pad="49"/>
<connect gate="-GND" pin="GND@8" pad="57"/>
<connect gate="-GND" pin="GND@9" pad="60"/>
<connect gate="-VCC" pin="VCC" pad="1"/>
<connect gate="-VCC" pin="VCC@1" pad="9"/>
<connect gate="-VCC" pin="VCC@10" pad="66"/>
<connect gate="-VCC" pin="VCC@11" pad="67"/>
<connect gate="-VCC" pin="VCC@12" pad="77"/>
<connect gate="-VCC" pin="VCC@13" pad="85"/>
<connect gate="-VCC" pin="VCC@14" pad="93"/>
<connect gate="-VCC" pin="VCC@15" pad="95"/>
<connect gate="-VCC" pin="VCC@16" pad="105"/>
<connect gate="-VCC" pin="VCC@17" pad="110"/>
<connect gate="-VCC" pin="VCC@18" pad="120"/>
<connect gate="-VCC" pin="VCC@19" pad="124"/>
<connect gate="-VCC" pin="VCC@2" pad="20"/>
<connect gate="-VCC" pin="VCC@20" pad="130"/>
<connect gate="-VCC" pin="VCC@21" pad="131"/>
<connect gate="-VCC" pin="VCC@22" pad="140"/>
<connect gate="-VCC" pin="VCC@23" pad="141"/>
<connect gate="-VCC" pin="VCC@24" pad="156"/>
<connect gate="-VCC" pin="VCC@25" pad="158"/>
<connect gate="-VCC" pin="VCC@26" pad="163"/>
<connect gate="-VCC" pin="VCC@27" pad="172"/>
<connect gate="-VCC" pin="VCC@28" pad="176"/>
<connect gate="-VCC" pin="VCC@29" pad="182"/>
<connect gate="-VCC" pin="VCC@3" pad="21"/>
<connect gate="-VCC" pin="VCC@30" pad="191"/>
<connect gate="-VCC" pin="VCC@31" pad="192"/>
<connect gate="-VCC" pin="VCC@32" pad="200"/>
<connect gate="-VCC" pin="VCC@4" pad="29"/>
<connect gate="-VCC" pin="VCC@5" pad="32"/>
<connect gate="-VCC" pin="VCC@6" pad="36"/>
<connect gate="-VCC" pin="VCC@7" pad="45"/>
<connect gate="-VCC" pin="VCC@8" pad="54"/>
<connect gate="-VCC" pin="VCC@9" pad="61"/>
<connect gate="G$1" pin="ACK" pad="69"/>
<connect gate="G$1" pin="ADDR0" pad="195"/>
<connect gate="G$1" pin="ADDR1" pad="194"/>
<connect gate="G$1" pin="ADDR10" pad="179"/>
<connect gate="G$1" pin="ADDR11" pad="178"/>
<connect gate="G$1" pin="ADDR12" pad="175"/>
<connect gate="G$1" pin="ADDR13" pad="174"/>
<connect gate="G$1" pin="ADDR14" pad="173"/>
<connect gate="G$1" pin="ADDR15" pad="171"/>
<connect gate="G$1" pin="ADDR16" pad="170"/>
<connect gate="G$1" pin="ADDR17" pad="169"/>
<connect gate="G$1" pin="ADDR18" pad="166"/>
<connect gate="G$1" pin="ADDR19" pad="165"/>
<connect gate="G$1" pin="ADDR2" pad="193"/>
<connect gate="G$1" pin="ADDR20" pad="164"/>
<connect gate="G$1" pin="ADDR21" pad="162"/>
<connect gate="G$1" pin="ADDR22" pad="161"/>
<connect gate="G$1" pin="ADDR23" pad="160"/>
<connect gate="G$1" pin="ADDR3" pad="190"/>
<connect gate="G$1" pin="ADDR4" pad="189"/>
<connect gate="G$1" pin="ADDR5" pad="188"/>
<connect gate="G$1" pin="ADDR6" pad="185"/>
<connect gate="G$1" pin="ADDR7" pad="184"/>
<connect gate="G$1" pin="ADDR8" pad="183"/>
<connect gate="G$1" pin="ADDR9" pad="180"/>
<connect gate="G$1" pin="BMS/" pad="153"/>
<connect gate="G$1" pin="BMSTR" pad="53"/>
<connect gate="G$1" pin="BR1/" pad="27"/>
<connect gate="G$1" pin="BR2/" pad="28"/>
<connect gate="G$1" pin="BSEL" pad="152"/>
<connect gate="G$1" pin="CAS/" pad="43"/>
<connect gate="G$1" pin="CLKIN" pad="30"/>
<connect gate="G$1" pin="CPA/" pad="65"/>
<connect gate="G$1" pin="CS/" pad="55"/>
<connect gate="G$1" pin="DATA0" pad="82"/>
<connect gate="G$1" pin="DATA1" pad="83"/>
<connect gate="G$1" pin="DATA10" pad="97"/>
<connect gate="G$1" pin="DATA11" pad="98"/>
<connect gate="G$1" pin="DATA12" pad="100"/>
<connect gate="G$1" pin="DATA13" pad="101"/>
<connect gate="G$1" pin="DATA14" pad="104"/>
<connect gate="G$1" pin="DATA15" pad="107"/>
<connect gate="G$1" pin="DATA16" pad="108"/>
<connect gate="G$1" pin="DATA17" pad="109"/>
<connect gate="G$1" pin="DATA18" pad="111"/>
<connect gate="G$1" pin="DATA19" pad="112"/>
<connect gate="G$1" pin="DATA2" pad="84"/>
<connect gate="G$1" pin="DATA20" pad="113"/>
<connect gate="G$1" pin="DATA21" pad="116"/>
<connect gate="G$1" pin="DATA22" pad="117"/>
<connect gate="G$1" pin="DATA23" pad="118"/>
<connect gate="G$1" pin="DATA24" pad="121"/>
<connect gate="G$1" pin="DATA25" pad="122"/>
<connect gate="G$1" pin="DATA26" pad="123"/>
<connect gate="G$1" pin="DATA27" pad="126"/>
<connect gate="G$1" pin="DATA28" pad="127"/>
<connect gate="G$1" pin="DATA29" pad="128"/>
<connect gate="G$1" pin="DATA3" pad="86"/>
<connect gate="G$1" pin="DATA30" pad="132"/>
<connect gate="G$1" pin="DATA31" pad="133"/>
<connect gate="G$1" pin="DATA4" pad="87"/>
<connect gate="G$1" pin="DATA5" pad="88"/>
<connect gate="G$1" pin="DATA6" pad="90"/>
<connect gate="G$1" pin="DATA7" pad="91"/>
<connect gate="G$1" pin="DATA8" pad="92"/>
<connect gate="G$1" pin="DATA9" pad="96"/>
<connect gate="G$1" pin="DMAG1/" pad="50"/>
<connect gate="G$1" pin="DMAG2/" pad="51"/>
<connect gate="G$1" pin="DMAR1/" pad="38"/>
<connect gate="G$1" pin="DMAR2/" pad="39"/>
<connect gate="G$1" pin="DQM/" pad="46"/>
<connect gate="G$1" pin="DR0A" pad="5"/>
<connect gate="G$1" pin="DR0B" pad="6"/>
<connect gate="G$1" pin="DR1A" pad="16"/>
<connect gate="G$1" pin="DR1B" pad="17"/>
<connect gate="G$1" pin="DT0A" pad="11"/>
<connect gate="G$1" pin="DT0B" pad="12"/>
<connect gate="G$1" pin="DT1A" pad="22"/>
<connect gate="G$1" pin="DT1B" pad="23"/>
<connect gate="G$1" pin="EMU/" pad="145"/>
<connect gate="G$1" pin="FLAG0" pad="197"/>
<connect gate="G$1" pin="FLAG1" pad="198"/>
<connect gate="G$1" pin="FLAG10" pad="78"/>
<connect gate="G$1" pin="FLAG11" pad="76"/>
<connect gate="G$1" pin="FLAG2" pad="199"/>
<connect gate="G$1" pin="FLAG3" pad="201"/>
<connect gate="G$1" pin="FLAG4" pad="138"/>
<connect gate="G$1" pin="FLAG5" pad="137"/>
<connect gate="G$1" pin="FLAG6" pad="136"/>
<connect gate="G$1" pin="FLAG7" pad="134"/>
<connect gate="G$1" pin="FLAG8" pad="80"/>
<connect gate="G$1" pin="FLAG9" pad="79"/>
<connect gate="G$1" pin="HBG/" pad="52"/>
<connect gate="G$1" pin="HBR/" pad="40"/>
<connect gate="G$1" pin="ID0" pad="144"/>
<connect gate="G$1" pin="ID1" pad="143"/>
<connect gate="G$1" pin="IRQ0/" pad="205"/>
<connect gate="G$1" pin="IRQ1/" pad="206"/>
<connect gate="G$1" pin="IRQ2/" pad="207"/>
<connect gate="G$1" pin="MS0/" pad="70"/>
<connect gate="G$1" pin="MS1/" pad="71"/>
<connect gate="G$1" pin="MS2/" pad="74"/>
<connect gate="G$1" pin="MS3/" pad="75"/>
<connect gate="G$1" pin="PWM_EVENT0" pad="26"/>
<connect gate="G$1" pin="PWM_EVENT1" pad="24"/>
<connect gate="G$1" pin="RAS/" pad="42"/>
<connect gate="G$1" pin="RCLK0" pad="4"/>
<connect gate="G$1" pin="RCLK1" pad="15"/>
<connect gate="G$1" pin="RD/" pad="59"/>
<connect gate="G$1" pin="REDY/" pad="63"/>
<connect gate="G$1" pin="RESET/" pad="157"/>
<connect gate="G$1" pin="RFS0" pad="2"/>
<connect gate="G$1" pin="RFS1" pad="13"/>
<connect gate="G$1" pin="SBTS/" pad="56"/>
<connect gate="G$1" pin="SDA10" pad="48"/>
<connect gate="G$1" pin="SDCKE" pad="47"/>
<connect gate="G$1" pin="SDCLK0" pad="37"/>
<connect gate="G$1" pin="SDCLK1" pad="34"/>
<connect gate="G$1" pin="SDWE/" pad="44"/>
<connect gate="G$1" pin="SW/" pad="64"/>
<connect gate="G$1" pin="TCK" pad="151"/>
<connect gate="G$1" pin="TCLK0" pad="8"/>
<connect gate="G$1" pin="TCLK1" pad="19"/>
<connect gate="G$1" pin="TDI" pad="148"/>
<connect gate="G$1" pin="TDO" pad="146"/>
<connect gate="G$1" pin="TFS0" pad="7"/>
<connect gate="G$1" pin="TFS1" pad="18"/>
<connect gate="G$1" pin="TMS" pad="149"/>
<connect gate="G$1" pin="TRST/" pad="147"/>
<connect gate="G$1" pin="WR/" pad="58"/>
<connect gate="G$1" pin="XTAL/" pad="31"/>
<connect gate="NC1" pin="NC" pad="102"/>
<connect gate="NC2" pin="NC" pad="103"/>
<connect gate="NC3" pin="NC" pad="115"/>
<connect gate="NC4" pin="NC" pad="142"/>
<connect gate="NC5" pin="NC" pad="202"/>
<connect gate="NC6" pin="NC" pad="203"/>
<connect gate="NC7" pin="NC" pad="208"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADP3303" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADP3303"/>
</gates>
<devices>
<device name="" package="SO8-COOL">
<connects>
<connect gate="G$1" pin="ERR/" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="IN@1" pad="7"/>
<connect gate="G$1" pin="NR" pad="3"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="OUT@2" pad="2"/>
<connect gate="G$1" pin="SC/" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADP3303ARZ-5"/>
<attribute name="OC_FARNELL" value="1465451"/>
<attribute name="OC_NEWARK" value="19M8716"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SP21060" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="-A" symbol="SP21060C"/>
<gate name="-B" symbol="A31"/>
<gate name="-C" symbol="D47"/>
<gate name="-D" symbol="L0"/>
<gate name="-E" symbol="L1"/>
<gate name="-F" symbol="L2"/>
<gate name="-G" symbol="L3"/>
<gate name="-H" symbol="L4"/>
<gate name="-I" symbol="L5"/>
<gate name="-VCC" symbol="VCC29"/>
<gate name="-GND" symbol="GND31"/>
<gate name="NC129" symbol="NC"/>
<gate name="NC203" symbol="NC"/>
</gates>
<devices>
<device name="" package="PQFP240">
<connects>
<connect gate="-A" pin="ACK" pad="99"/>
<connect gate="-A" pin="ADRCLK" pad="89"/>
<connect gate="-A" pin="BMS/" pad="59"/>
<connect gate="-A" pin="BR1/" pad="109"/>
<connect gate="-A" pin="BR2/" pad="108"/>
<connect gate="-A" pin="BR3/" pad="107"/>
<connect gate="-A" pin="BR4/" pad="106"/>
<connect gate="-A" pin="BR5/" pad="105"/>
<connect gate="-A" pin="BR6/" pad="104"/>
<connect gate="-A" pin="CLKIN" pad="98"/>
<connect gate="-A" pin="CPA/" pad="79"/>
<connect gate="-A" pin="CS/" pad="92"/>
<connect gate="-A" pin="DMAG1/" pad="101"/>
<connect gate="-A" pin="DMAG2/" pad="100"/>
<connect gate="-A" pin="DMAR1/" pad="70"/>
<connect gate="-A" pin="DMAR2/" pad="69"/>
<connect gate="-A" pin="DR0" pad="83"/>
<connect gate="-A" pin="DR1" pad="75"/>
<connect gate="-A" pin="DT0" pad="80"/>
<connect gate="-A" pin="DT1" pad="72"/>
<connect gate="-A" pin="EBOOT" pad="235"/>
<connect gate="-A" pin="EMU/" pad="6"/>
<connect gate="-A" pin="FLAG0" pad="11"/>
<connect gate="-A" pin="FLAG1" pad="10"/>
<connect gate="-A" pin="FLAG2" pad="9"/>
<connect gate="-A" pin="FLAG3" pad="8"/>
<connect gate="-A" pin="HBG/" pad="91"/>
<connect gate="-A" pin="HBR/" pad="71"/>
<connect gate="-A" pin="ICSA" pad="7"/>
<connect gate="-A" pin="ID0" pad="231"/>
<connect gate="-A" pin="ID1" pad="230"/>
<connect gate="-A" pin="ID2" pad="229"/>
<connect gate="-A" pin="IRQ0/" pad="238"/>
<connect gate="-A" pin="IRQ1/" pad="237"/>
<connect gate="-A" pin="IRQ2/" pad="236"/>
<connect gate="-A" pin="LBOOT" pad="232"/>
<connect gate="-A" pin="MS0/" pad="57"/>
<connect gate="-A" pin="MS1/" pad="56"/>
<connect gate="-A" pin="MS2/" pad="55"/>
<connect gate="-A" pin="MS3/" pad="54"/>
<connect gate="-A" pin="PAGE" pad="102"/>
<connect gate="-A" pin="RCLK0" pad="84"/>
<connect gate="-A" pin="RCLK1" pad="76"/>
<connect gate="-A" pin="RD/" pad="93"/>
<connect gate="-A" pin="REDY/" pad="90"/>
<connect gate="-A" pin="RESET/" pad="234"/>
<connect gate="-A" pin="RFS0" pad="85"/>
<connect gate="-A" pin="RFS1" pad="77"/>
<connect gate="-A" pin="RPBA" pad="233"/>
<connect gate="-A" pin="SBTS/" pad="68"/>
<connect gate="-A" pin="SW/" pad="58"/>
<connect gate="-A" pin="TCK" pad="239"/>
<connect gate="-A" pin="TCLK0" pad="81"/>
<connect gate="-A" pin="TCLK1" pad="73"/>
<connect gate="-A" pin="TDI" pad="1"/>
<connect gate="-A" pin="TDO" pad="4"/>
<connect gate="-A" pin="TFS0" pad="82"/>
<connect gate="-A" pin="TFS1" pad="74"/>
<connect gate="-A" pin="TIMEXP" pad="5"/>
<connect gate="-A" pin="TMS" pad="240"/>
<connect gate="-A" pin="TRST/" pad="2"/>
<connect gate="-A" pin="WR/_" pad="94"/>
<connect gate="-B" pin="A0" pad="13"/>
<connect gate="-B" pin="A1" pad="14"/>
<connect gate="-B" pin="A10" pad="26"/>
<connect gate="-B" pin="A11" pad="28"/>
<connect gate="-B" pin="A12" pad="29"/>
<connect gate="-B" pin="A13" pad="30"/>
<connect gate="-B" pin="A14" pad="32"/>
<connect gate="-B" pin="A15" pad="33"/>
<connect gate="-B" pin="A16" pad="35"/>
<connect gate="-B" pin="A17" pad="36"/>
<connect gate="-B" pin="A18" pad="37"/>
<connect gate="-B" pin="A19" pad="40"/>
<connect gate="-B" pin="A2" pad="16"/>
<connect gate="-B" pin="A20" pad="41"/>
<connect gate="-B" pin="A21" pad="42"/>
<connect gate="-B" pin="A22" pad="44"/>
<connect gate="-B" pin="A23" pad="45"/>
<connect gate="-B" pin="A24" pad="46"/>
<connect gate="-B" pin="A25" pad="50"/>
<connect gate="-B" pin="A26" pad="51"/>
<connect gate="-B" pin="A27" pad="52"/>
<connect gate="-B" pin="A28" pad="60"/>
<connect gate="-B" pin="A29" pad="64"/>
<connect gate="-B" pin="A3" pad="17"/>
<connect gate="-B" pin="A30" pad="65"/>
<connect gate="-B" pin="A31" pad="66"/>
<connect gate="-B" pin="A4" pad="18"/>
<connect gate="-B" pin="A5" pad="20"/>
<connect gate="-B" pin="A6" pad="21"/>
<connect gate="-B" pin="A7" pad="22"/>
<connect gate="-B" pin="A8" pad="24"/>
<connect gate="-B" pin="A9" pad="25"/>
<connect gate="-C" pin="D0" pad="179"/>
<connect gate="-C" pin="D1" pad="178"/>
<connect gate="-C" pin="D10" pad="166"/>
<connect gate="-C" pin="D11" pad="165"/>
<connect gate="-C" pin="D12" pad="163"/>
<connect gate="-C" pin="D13" pad="162"/>
<connect gate="-C" pin="D14" pad="161"/>
<connect gate="-C" pin="D15" pad="159"/>
<connect gate="-C" pin="D16" pad="158"/>
<connect gate="-C" pin="D17" pad="157"/>
<connect gate="-C" pin="D18" pad="155"/>
<connect gate="-C" pin="D19" pad="154"/>
<connect gate="-C" pin="D2" pad="177"/>
<connect gate="-C" pin="D20" pad="153"/>
<connect gate="-C" pin="D21" pad="151"/>
<connect gate="-C" pin="D22" pad="150"/>
<connect gate="-C" pin="D23" pad="149"/>
<connect gate="-C" pin="D24" pad="147"/>
<connect gate="-C" pin="D25" pad="146"/>
<connect gate="-C" pin="D26" pad="145"/>
<connect gate="-C" pin="D27" pad="142"/>
<connect gate="-C" pin="D28" pad="141"/>
<connect gate="-C" pin="D29" pad="140"/>
<connect gate="-C" pin="D3" pad="175"/>
<connect gate="-C" pin="D30" pad="138"/>
<connect gate="-C" pin="D31" pad="137"/>
<connect gate="-C" pin="D32" pad="136"/>
<connect gate="-C" pin="D33" pad="132"/>
<connect gate="-C" pin="D34" pad="131"/>
<connect gate="-C" pin="D35" pad="130"/>
<connect gate="-C" pin="D36" pad="127"/>
<connect gate="-C" pin="D37" pad="126"/>
<connect gate="-C" pin="D38" pad="125"/>
<connect gate="-C" pin="D39" pad="123"/>
<connect gate="-C" pin="D4" pad="174"/>
<connect gate="-C" pin="D40" pad="122"/>
<connect gate="-C" pin="D41" pad="121"/>
<connect gate="-C" pin="D42" pad="119"/>
<connect gate="-C" pin="D43" pad="118"/>
<connect gate="-C" pin="D44" pad="117"/>
<connect gate="-C" pin="D45" pad="115"/>
<connect gate="-C" pin="D46" pad="114"/>
<connect gate="-C" pin="D47" pad="113"/>
<connect gate="-C" pin="D5" pad="173"/>
<connect gate="-C" pin="D6" pad="171"/>
<connect gate="-C" pin="D7" pad="170"/>
<connect gate="-C" pin="D8" pad="169"/>
<connect gate="-C" pin="D9" pad="167"/>
<connect gate="-D" pin="L0ACK" pad="187"/>
<connect gate="-D" pin="L0CLK" pad="186"/>
<connect gate="-D" pin="L0DAT0" pad="185"/>
<connect gate="-D" pin="L0DAT1" pad="184"/>
<connect gate="-D" pin="L0DAT2" pad="183"/>
<connect gate="-D" pin="L0DAT3" pad="182"/>
<connect gate="-E" pin="L1ACK" pad="194"/>
<connect gate="-E" pin="L1CLK" pad="193"/>
<connect gate="-E" pin="L1DAT0" pad="192"/>
<connect gate="-E" pin="L1DAT1" pad="191"/>
<connect gate="-E" pin="L1DAT2" pad="190"/>
<connect gate="-E" pin="L1DAT3" pad="189"/>
<connect gate="-F" pin="L2ACK" pad="202"/>
<connect gate="-F" pin="L2CLK" pad="201"/>
<connect gate="-F" pin="L2DAT0" pad="200"/>
<connect gate="-F" pin="L2DAT1" pad="199"/>
<connect gate="-F" pin="L2DAT2" pad="198"/>
<connect gate="-F" pin="L2DAT3" pad="197"/>
<connect gate="-G" pin="L3ACK" pad="210"/>
<connect gate="-G" pin="L3CLK" pad="209"/>
<connect gate="-G" pin="L3DAT0" pad="208"/>
<connect gate="-G" pin="L3DAT1" pad="207"/>
<connect gate="-G" pin="L3DAT2" pad="206"/>
<connect gate="-G" pin="L3DAT3" pad="205"/>
<connect gate="-GND" pin="GND" pad="12"/>
<connect gate="-GND" pin="GND@1" pad="19"/>
<connect gate="-GND" pin="GND@10" pad="88"/>
<connect gate="-GND" pin="GND@11" pad="95"/>
<connect gate="-GND" pin="GND@12" pad="97"/>
<connect gate="-GND" pin="GND@13" pad="110"/>
<connect gate="-GND" pin="GND@14" pad="112"/>
<connect gate="-GND" pin="GND@15" pad="120"/>
<connect gate="-GND" pin="GND@16" pad="128"/>
<connect gate="-GND" pin="GND@17" pad="135"/>
<connect gate="-GND" pin="GND@18" pad="139"/>
<connect gate="-GND" pin="GND@19" pad="148"/>
<connect gate="-GND" pin="GND@2" pad="27"/>
<connect gate="-GND" pin="GND@20" pad="156"/>
<connect gate="-GND" pin="GND@21" pad="164"/>
<connect gate="-GND" pin="GND@22" pad="172"/>
<connect gate="-GND" pin="GND@23" pad="180"/>
<connect gate="-GND" pin="GND@24" pad="181"/>
<connect gate="-GND" pin="GND@25" pad="195"/>
<connect gate="-GND" pin="GND@26" pad="196"/>
<connect gate="-GND" pin="GND@27" pad="211"/>
<connect gate="-GND" pin="GND@28" pad="212"/>
<connect gate="-GND" pin="GND@29" pad="220"/>
<connect gate="-GND" pin="GND@3" pad="34"/>
<connect gate="-GND" pin="GND@30" pad="228"/>
<connect gate="-GND" pin="GND@4" pad="43"/>
<connect gate="-GND" pin="GND@5" pad="48"/>
<connect gate="-GND" pin="GND@6" pad="53"/>
<connect gate="-GND" pin="GND@7" pad="61"/>
<connect gate="-GND" pin="GND@8" pad="67"/>
<connect gate="-GND" pin="GND@9" pad="78"/>
<connect gate="-H" pin="L4ACK" pad="218"/>
<connect gate="-H" pin="L4CLK" pad="217"/>
<connect gate="-H" pin="L4DAT0" pad="216"/>
<connect gate="-H" pin="L4DAT1" pad="215"/>
<connect gate="-H" pin="L4DAT2" pad="214"/>
<connect gate="-H" pin="L4DAT3" pad="213"/>
<connect gate="-I" pin="L5ACK" pad="227"/>
<connect gate="-I" pin="L5CLK" pad="226"/>
<connect gate="-I" pin="L5DAT0" pad="225"/>
<connect gate="-I" pin="L5DAT1" pad="224"/>
<connect gate="-I" pin="L5DAT2" pad="223"/>
<connect gate="-I" pin="L5DAT3" pad="222"/>
<connect gate="-VCC" pin="VCC" pad="3"/>
<connect gate="-VCC" pin="VCC@1" pad="15"/>
<connect gate="-VCC" pin="VCC@10" pad="86"/>
<connect gate="-VCC" pin="VCC@11" pad="87"/>
<connect gate="-VCC" pin="VCC@12" pad="96"/>
<connect gate="-VCC" pin="VCC@13" pad="103"/>
<connect gate="-VCC" pin="VCC@14" pad="111"/>
<connect gate="-VCC" pin="VCC@15" pad="116"/>
<connect gate="-VCC" pin="VCC@16" pad="124"/>
<connect gate="-VCC" pin="VCC@17" pad="133"/>
<connect gate="-VCC" pin="VCC@18" pad="134"/>
<connect gate="-VCC" pin="VCC@19" pad="143"/>
<connect gate="-VCC" pin="VCC@2" pad="23"/>
<connect gate="-VCC" pin="VCC@20" pad="144"/>
<connect gate="-VCC" pin="VCC@21" pad="152"/>
<connect gate="-VCC" pin="VCC@22" pad="160"/>
<connect gate="-VCC" pin="VCC@23" pad="168"/>
<connect gate="-VCC" pin="VCC@24" pad="176"/>
<connect gate="-VCC" pin="VCC@25" pad="188"/>
<connect gate="-VCC" pin="VCC@26" pad="204"/>
<connect gate="-VCC" pin="VCC@27" pad="219"/>
<connect gate="-VCC" pin="VCC@28" pad="221"/>
<connect gate="-VCC" pin="VCC@3" pad="31"/>
<connect gate="-VCC" pin="VCC@4" pad="38"/>
<connect gate="-VCC" pin="VCC@5" pad="39"/>
<connect gate="-VCC" pin="VCC@6" pad="47"/>
<connect gate="-VCC" pin="VCC@7" pad="49"/>
<connect gate="-VCC" pin="VCC@8" pad="62"/>
<connect gate="-VCC" pin="VCC@9" pad="63"/>
<connect gate="NC129" pin="NC" pad="129"/>
<connect gate="NC203" pin="NC" pad="203"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADSP-21060KSZ-133"/>
<attribute name="OC_FARNELL" value="1438767"/>
<attribute name="OC_NEWARK" value="46M5216"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC812" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADUC812"/>
</gates>
<devices>
<device name="" package="PQFP52">
<connects>
<connect gate="G$1" pin="!EA" pad="40"/>
<connect gate="G$1" pin="!PSEN" pad="41"/>
<connect gate="G$1" pin="A10-A18" pad="30"/>
<connect gate="G$1" pin="A11-A19" pad="31"/>
<connect gate="G$1" pin="A12-A20" pad="36"/>
<connect gate="G$1" pin="A13-A21" pad="37"/>
<connect gate="G$1" pin="A14-A22" pad="38"/>
<connect gate="G$1" pin="A15-A23" pad="39"/>
<connect gate="G$1" pin="A8-A16" pad="28"/>
<connect gate="G$1" pin="A9-A17" pad="29"/>
<connect gate="G$1" pin="ADC0/T2" pad="1"/>
<connect gate="G$1" pin="ADC1/T2EX" pad="2"/>
<connect gate="G$1" pin="ADC2" pad="3"/>
<connect gate="G$1" pin="ADC3" pad="4"/>
<connect gate="G$1" pin="ADC4" pad="11"/>
<connect gate="G$1" pin="ADC5/!SS" pad="12"/>
<connect gate="G$1" pin="ADC6" pad="13"/>
<connect gate="G$1" pin="ADC7" pad="14"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="ALE" pad="42"/>
<connect gate="G$1" pin="AVDD" pad="5"/>
<connect gate="G$1" pin="CREF" pad="7"/>
<connect gate="G$1" pin="D@GND1" pad="35"/>
<connect gate="G$1" pin="DAC0" pad="9"/>
<connect gate="G$1" pin="DAC1" pad="10"/>
<connect gate="G$1" pin="DGND" pad="21"/>
<connect gate="G$1" pin="DGND@2" pad="47"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="DVDD@1" pad="34"/>
<connect gate="G$1" pin="DVDD@2" pad="48"/>
<connect gate="G$1" pin="P0.0/AD0" pad="43"/>
<connect gate="G$1" pin="P0.1/AD1" pad="44"/>
<connect gate="G$1" pin="P0.2/AD2" pad="45"/>
<connect gate="G$1" pin="P0.3/AD3" pad="46"/>
<connect gate="G$1" pin="P0.4/AD4" pad="49"/>
<connect gate="G$1" pin="P0.5/AD5" pad="50"/>
<connect gate="G$1" pin="P0.6/AD6" pad="51"/>
<connect gate="G$1" pin="P0.7/AD7" pad="52"/>
<connect gate="G$1" pin="P3.0/RXD" pad="16"/>
<connect gate="G$1" pin="P3.1/TXD" pad="17"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="18"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="19"/>
<connect gate="G$1" pin="P3.4/T0" pad="22"/>
<connect gate="G$1" pin="P3.5/T1" pad="23"/>
<connect gate="G$1" pin="P3.6/!WR" pad="24"/>
<connect gate="G$1" pin="P3.7/!RD" pad="25"/>
<connect gate="G$1" pin="RESET" pad="15"/>
<connect gate="G$1" pin="SCLOCK" pad="26"/>
<connect gate="G$1" pin="SDATA/MOSI" pad="27"/>
<connect gate="G$1" pin="VREF" pad="8"/>
<connect gate="G$1" pin="XTAL1" pad="32"/>
<connect gate="G$1" pin="XTAL2" pad="33"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADUC812BSZ"/>
<attribute name="OC_FARNELL" value="9605282"/>
<attribute name="OC_NEWARK" value="59K3130"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD102" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD102"/>
</gates>
<devices>
<device name="" package="AD102">
<connects>
<connect gate="G$1" pin="+15V_DC" pad="7"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="ICOM" pad="4"/>
<connect gate="G$1" pin="IN+" pad="5"/>
<connect gate="G$1" pin="IN-" pad="6"/>
<connect gate="G$1" pin="OUT_HI" pad="1"/>
<connect gate="G$1" pin="OUT_LO" pad="9"/>
<connect gate="G$1" pin="PWRCOM" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD104" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD104"/>
</gates>
<devices>
<device name="" package="AD104">
<connects>
<connect gate="G$1" pin="CLK_IN" pad="8"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="ICOM" pad="4"/>
<connect gate="G$1" pin="IN+" pad="5"/>
<connect gate="G$1" pin="IN-" pad="6"/>
<connect gate="G$1" pin="OUT_HI" pad="1"/>
<connect gate="G$1" pin="OUT_LO" pad="9"/>
<connect gate="G$1" pin="PWRCOM" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD1047"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="27R0347"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD767" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD767"/>
</gates>
<devices>
<device name="" package="DIL24-3">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="10V" pad="2"/>
<connect gate="G$1" pin="20V" pad="1"/>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="B_OFFSET" pad="4"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D10" pad="23"/>
<connect gate="G$1" pin="D11" pad="24"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="16"/>
<connect gate="G$1" pin="D4" pad="17"/>
<connect gate="G$1" pin="D5" pad="18"/>
<connect gate="G$1" pin="D6" pad="19"/>
<connect gate="G$1" pin="D7" pad="20"/>
<connect gate="G$1" pin="D8" pad="21"/>
<connect gate="G$1" pin="D9" pad="22"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="REF_IN" pad="7"/>
<connect gate="G$1" pin="REF_OUT" pad="6"/>
<connect gate="G$1" pin="SUM_JCT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VEE" pad="10"/>
<connect gate="G$1" pin="VOUT" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD767KNZ"/>
<attribute name="OC_FARNELL" value="9604510"/>
<attribute name="OC_NEWARK" value="59K5176"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD736R" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD736"/>
</gates>
<devices>
<device name="" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="CAV" pad="5"/>
<connect gate="G$1" pin="CC" pad="1"/>
<connect gate="G$1" pin="CF" pad="3"/>
<connect gate="G$1" pin="COM" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD736JRZ"/>
<attribute name="OC_FARNELL" value="1701156"/>
<attribute name="OC_NEWARK" value="19M0863"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD736N" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD736"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="CAV" pad="5"/>
<connect gate="G$1" pin="CC" pad="1"/>
<connect gate="G$1" pin="CF" pad="3"/>
<connect gate="G$1" pin="COM" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD736JN"/>
<attribute name="OC_FARNELL" value="9605061"/>
<attribute name="OC_NEWARK" value="05F7334"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD536ASE" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD536"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
</gates>
<devices>
<device name="" package="LCC20">
<connects>
<connect gate="G$1" pin="+VS" pad="20"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="BIN" pad="10"/>
<connect gate="G$1" pin="BOUT" pad="9"/>
<connect gate="G$1" pin="CAV" pad="6"/>
<connect gate="G$1" pin="COM" pad="14"/>
<connect gate="G$1" pin="DB" pad="8"/>
<connect gate="G$1" pin="IOUT" pad="12"/>
<connect gate="G$1" pin="RL" pad="13"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="19"/>
<connect gate="NC2" pin="NC" pad="3"/>
<connect gate="NC3" pin="NC" pad="5"/>
<connect gate="NC4" pin="NC" pad="7"/>
<connect gate="NC5" pin="NC" pad="11"/>
<connect gate="NC6" pin="NC" pad="15"/>
<connect gate="NC7" pin="NC" pad="16"/>
<connect gate="NC8" pin="NC" pad="17"/>
<connect gate="NC9" pin="NC" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD536AJH" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD536"/>
</gates>
<devices>
<device name="" package="TO100">
<connects>
<connect gate="G$1" pin="+VS" pad="3"/>
<connect gate="G$1" pin="-VS" pad="5"/>
<connect gate="G$1" pin="BIN" pad="9"/>
<connect gate="G$1" pin="BOUT" pad="8"/>
<connect gate="G$1" pin="CAV" pad="6"/>
<connect gate="G$1" pin="COM" pad="2"/>
<connect gate="G$1" pin="DB" pad="7"/>
<connect gate="G$1" pin="IOUT" pad="10"/>
<connect gate="G$1" pin="RL" pad="1"/>
<connect gate="G$1" pin="VIN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD536AJH"/>
<attribute name="OC_FARNELL" value="405360"/>
<attribute name="OC_NEWARK" value="05F6940"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD536AJD" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD536"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+VS" pad="14"/>
<connect gate="G$1" pin="-VS" pad="3"/>
<connect gate="G$1" pin="BIN" pad="7"/>
<connect gate="G$1" pin="BOUT" pad="6"/>
<connect gate="G$1" pin="CAV" pad="4"/>
<connect gate="G$1" pin="COM" pad="10"/>
<connect gate="G$1" pin="DB" pad="5"/>
<connect gate="G$1" pin="IOUT" pad="8"/>
<connect gate="G$1" pin="RL" pad="9"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="NC1" pin="NC" pad="2"/>
<connect gate="NC2" pin="NC" pad="11"/>
<connect gate="NC3" pin="NC" pad="12"/>
<connect gate="NC4" pin="NC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD536AJD"/>
<attribute name="OC_FARNELL" value="405358"/>
<attribute name="OC_NEWARK" value="05F6939"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD595" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD595"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+ALM" pad="12"/>
<connect gate="G$1" pin="+C" pad="2"/>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+T" pad="3"/>
<connect gate="G$1" pin="-ALM" pad="13"/>
<connect gate="G$1" pin="-C" pad="6"/>
<connect gate="G$1" pin="-IN" pad="14"/>
<connect gate="G$1" pin="-T" pad="5"/>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="COMP" pad="10"/>
<connect gate="G$1" pin="FB" pad="8"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VO" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD595AQ"/>
<attribute name="OC_FARNELL" value="409194"/>
<attribute name="OC_NEWARK" value="06WX1596"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD594" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD595"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+ALM" pad="12"/>
<connect gate="G$1" pin="+C" pad="2"/>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+T" pad="3"/>
<connect gate="G$1" pin="-ALM" pad="13"/>
<connect gate="G$1" pin="-C" pad="6"/>
<connect gate="G$1" pin="-IN" pad="14"/>
<connect gate="G$1" pin="-T" pad="5"/>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="COMP" pad="10"/>
<connect gate="G$1" pin="FB" pad="8"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="7"/>
<connect gate="G$1" pin="VO" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD594AQ"/>
<attribute name="OC_FARNELL" value="409182"/>
<attribute name="OC_NEWARK" value="05F7088"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8801" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD8801"/>
</gates>
<devices>
<device name="" package="SOIC16N">
<connects>
<connect gate="G$1" pin="!CLK" pad="9"/>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="!RS" pad="15"/>
<connect gate="G$1" pin="!SHDN" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="O1" pad="2"/>
<connect gate="G$1" pin="O2" pad="3"/>
<connect gate="G$1" pin="O3" pad="4"/>
<connect gate="G$1" pin="O4" pad="5"/>
<connect gate="G$1" pin="O5" pad="11"/>
<connect gate="G$1" pin="O6" pad="12"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="14"/>
<connect gate="G$1" pin="SDI" pad="10"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREFH" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8803" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD8803"/>
</gates>
<devices>
<device name="" package="SOIC16N">
<connects>
<connect gate="G$1" pin="!CLK" pad="10"/>
<connect gate="G$1" pin="!CS" pad="7"/>
<connect gate="G$1" pin="!SHDN" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="O1" pad="2"/>
<connect gate="G$1" pin="O2" pad="3"/>
<connect gate="G$1" pin="O3" pad="4"/>
<connect gate="G$1" pin="O4" pad="5"/>
<connect gate="G$1" pin="O5" pad="12"/>
<connect gate="G$1" pin="O6" pad="13"/>
<connect gate="G$1" pin="O7" pad="14"/>
<connect gate="G$1" pin="O8" pad="15"/>
<connect gate="G$1" pin="SDI" pad="11"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREFH" pad="1"/>
<connect gate="G$1" pin="VREFL" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD811_SO8" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
<gate name="1" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="8" symbol="NC"/>
</gates>
<devices>
<device name="" package="SO8">
<connects>
<connect gate="1" pin="NC" pad="1"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="8" pin="NC" pad="8"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD811JRZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="82H2980"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD811_N" prefix="IC" uservalue="yes">
<description>&lt;b&gt;ANALOG DEVICES&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
<gate name="1" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="8" symbol="NC"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="1" pin="NC" pad="1"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="8" pin="NC" pad="8"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD811ANZ"/>
<attribute name="OC_FARNELL" value="1464857"/>
<attribute name="OC_NEWARK" value="58K5191"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD538*" prefix="IC">
<description>&lt;b&gt;Real-Time Analog Computational Unit (ACU)&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD538"/>
</gates>
<devices>
<device name="D" package="DIL18">
<connects>
<connect gate="G$1" pin="+10V" pad="4"/>
<connect gate="G$1" pin="+2V" pad="5"/>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="-VS" pad="7"/>
<connect gate="G$1" pin="A" pad="18"/>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="12"/>
<connect gate="G$1" pin="D" pad="17"/>
<connect gate="G$1" pin="I" pad="9"/>
<connect gate="G$1" pin="IX" pad="16"/>
<connect gate="G$1" pin="IY" pad="11"/>
<connect gate="G$1" pin="IZ" pad="1"/>
<connect gate="G$1" pin="PWR_GND" pad="13"/>
<connect gate="G$1" pin="SIGNAL_GND" pad="14"/>
<connect gate="G$1" pin="VO" pad="8"/>
<connect gate="G$1" pin="VX" pad="15"/>
<connect gate="G$1" pin="VY" pad="10"/>
<connect gate="G$1" pin="VZ" pad="2"/>
</connects>
<technologies>
<technology name="A">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD538AD"/>
<attribute name="OC_FARNELL" value="402667"/>
<attribute name="OC_NEWARK" value="05F6949"/>
</technology>
<technology name="B">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD538BD"/>
<attribute name="OC_FARNELL" value="1530988"/>
<attribute name="OC_NEWARK" value="05F6950"/>
</technology>
<technology name="S">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD538SD"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16F3434"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD654" prefix="IC">
<description>&lt;b&gt;Low Cost Monolithic Voltage-to-Frequency Converter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD654"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+VIN" pad="4"/>
<connect gate="G$1" pin="+VS" pad="8"/>
<connect gate="G$1" pin="-VS" pad="5"/>
<connect gate="G$1" pin="CT1" pad="6"/>
<connect gate="G$1" pin="CT2" pad="7"/>
<connect gate="G$1" pin="FOUT" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD654JNZ/+"/>
<attribute name="OC_FARNELL" value="9605053"/>
<attribute name="OC_NEWARK" value="59K4466"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP2189M*" prefix="IC">
<description>&lt;b&gt;DSP Microcomputer&lt;/b&gt;&lt;p&gt;
single-chip microcomputer optimized for digital signal processing (DSP)</description>
<gates>
<gate name="G$1" symbol="ADSP2189"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="G$1" pin="!BGH" pad="95"/>
<connect gate="G$1" pin="!BMS" pad="21"/>
<connect gate="G$1" pin="!BR" pad="52"/>
<connect gate="G$1" pin="!CMS" pad="25"/>
<connect gate="G$1" pin="!DMS" pad="22"/>
<connect gate="G$1" pin="!EBG" pad="53"/>
<connect gate="G$1" pin="!EBR" pad="51"/>
<connect gate="G$1" pin="!EINT" pad="50"/>
<connect gate="G$1" pin="!EMS" pad="45"/>
<connect gate="G$1" pin="!ERESET" pad="43"/>
<connect gate="G$1" pin="!IACK!-D3" pad="58"/>
<connect gate="G$1" pin="!IOMS" pad="24"/>
<connect gate="G$1" pin="!IRD!-D6" pad="63"/>
<connect gate="G$1" pin="!IRQ2!-PF7" pad="30"/>
<connect gate="G$1" pin="!IRQE!-PF4" pad="26"/>
<connect gate="G$1" pin="!IRQL0!-PF5" pad="27"/>
<connect gate="G$1" pin="!IRQL1!-PF6" pad="29"/>
<connect gate="G$1" pin="!IS!-D4" pad="61"/>
<connect gate="G$1" pin="!IWR!-D7" pad="64"/>
<connect gate="G$1" pin="!PMS" pad="23"/>
<connect gate="G$1" pin="!PWD" pad="91"/>
<connect gate="G$1" pin="!PWDACK" pad="96"/>
<connect gate="G$1" pin="!RD" pad="20"/>
<connect gate="G$1" pin="!RESET" pad="44"/>
<connect gate="G$1" pin="!RFS1!-IRQ0" pad="39"/>
<connect gate="G$1" pin="!TFS1!-IRQ1" pad="38"/>
<connect gate="G$1" pin="!WR" pad="19"/>
<connect gate="G$1" pin="A0" pad="97"/>
<connect gate="G$1" pin="BG" pad="54"/>
<connect gate="G$1" pin="CLKIN" pad="13"/>
<connect gate="G$1" pin="CLKOUT" pad="16"/>
<connect gate="G$1" pin="D10" pad="69"/>
<connect gate="G$1" pin="D11" pad="70"/>
<connect gate="G$1" pin="D12" pad="72"/>
<connect gate="G$1" pin="D13" pad="73"/>
<connect gate="G$1" pin="D14" pad="74"/>
<connect gate="G$1" pin="D15" pad="75"/>
<connect gate="G$1" pin="D16" pad="76"/>
<connect gate="G$1" pin="D17" pad="77"/>
<connect gate="G$1" pin="D18" pad="78"/>
<connect gate="G$1" pin="D19" pad="79"/>
<connect gate="G$1" pin="D20" pad="81"/>
<connect gate="G$1" pin="D21" pad="82"/>
<connect gate="G$1" pin="D22" pad="83"/>
<connect gate="G$1" pin="D23" pad="84"/>
<connect gate="G$1" pin="D8" pad="65"/>
<connect gate="G$1" pin="D9" pad="68"/>
<connect gate="G$1" pin="DR0" pad="34"/>
<connect gate="G$1" pin="DR1-FI" pad="40"/>
<connect gate="G$1" pin="DT0" pad="31"/>
<connect gate="G$1" pin="DT1-FO" pad="37"/>
<connect gate="G$1" pin="ECLK" pad="47"/>
<connect gate="G$1" pin="ECLKOUT" pad="48"/>
<connect gate="G$1" pin="EE" pad="46"/>
<connect gate="G$1" pin="ELIN" pad="49"/>
<connect gate="G$1" pin="FL0" pad="87"/>
<connect gate="G$1" pin="FL1" pad="86"/>
<connect gate="G$1" pin="FL2" pad="85"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="17"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="GND@4" pad="41"/>
<connect gate="G$1" pin="GND@5" pad="60"/>
<connect gate="G$1" pin="GND@6" pad="66"/>
<connect gate="G$1" pin="GND@7" pad="71"/>
<connect gate="G$1" pin="GND@8" pad="80"/>
<connect gate="G$1" pin="GND@9" pad="92"/>
<connect gate="G$1" pin="IAD0-A1" pad="98"/>
<connect gate="G$1" pin="IAD1-A2" pad="99"/>
<connect gate="G$1" pin="IAD10-A11" pad="9"/>
<connect gate="G$1" pin="IAD11-A12" pad="10"/>
<connect gate="G$1" pin="IAD12-A13" pad="11"/>
<connect gate="G$1" pin="IAD13-D0" pad="55"/>
<connect gate="G$1" pin="IAD14-D1" pad="56"/>
<connect gate="G$1" pin="IAD15-D2" pad="57"/>
<connect gate="G$1" pin="IAD2-A3" pad="100"/>
<connect gate="G$1" pin="IAD3-A4" pad="1"/>
<connect gate="G$1" pin="IAD4-A5" pad="2"/>
<connect gate="G$1" pin="IAD5-A6" pad="4"/>
<connect gate="G$1" pin="IAD6-A7" pad="5"/>
<connect gate="G$1" pin="IAD7-A8" pad="6"/>
<connect gate="G$1" pin="IAD8-A9" pad="7"/>
<connect gate="G$1" pin="IAD9-A10" pad="8"/>
<connect gate="G$1" pin="IAL-D5" pad="62"/>
<connect gate="G$1" pin="MODEA-PF0" pad="94"/>
<connect gate="G$1" pin="MODEB-PF1" pad="93"/>
<connect gate="G$1" pin="MODEC-PF2" pad="89"/>
<connect gate="G$1" pin="MODED-PF3" pad="88"/>
<connect gate="G$1" pin="RFS0" pad="33"/>
<connect gate="G$1" pin="SCLK0" pad="35"/>
<connect gate="G$1" pin="SCLK1" pad="42"/>
<connect gate="G$1" pin="TFS0" pad="32"/>
<connect gate="G$1" pin="VDDEXT" pad="15"/>
<connect gate="G$1" pin="VDDEXT@1" pad="36"/>
<connect gate="G$1" pin="VDDEXT@2" pad="67"/>
<connect gate="G$1" pin="VDDEXT@3" pad="90"/>
<connect gate="G$1" pin="VDDINT" pad="18"/>
<connect gate="G$1" pin="VDDINT@1" pad="59"/>
<connect gate="G$1" pin="XTAL" pad="14"/>
</connects>
<technologies>
<technology name="BST-266">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADSP-2189MBST-266"/>
<attribute name="OC_FARNELL" value="1465571"/>
<attribute name="OC_NEWARK" value="98B1516"/>
</technology>
<technology name="KST-300">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADSP-2189MKST-300"/>
<attribute name="OC_FARNELL" value="1465572"/>
<attribute name="OC_NEWARK" value="98B7141"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP21161" prefix="IC">
<description>&lt;b&gt;DSP Microcomputer&lt;/b&gt;</description>
<gates>
<gate name="E" symbol="ADSP-21161-ADR"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="B" symbol="ADSP-21161-CTRL1"/>
<gate name="A" symbol="ADSP-21161-CTRL2"/>
<gate name="C" symbol="ADSP-21161-PAR"/>
<gate name="D" symbol="ADSP-21161-SER"/>
<gate name="VE1" symbol="VDDEXT"/>
<gate name="VE2" symbol="VDDEXT"/>
<gate name="VE3" symbol="VDDEXT"/>
<gate name="VE4" symbol="VDDEXT"/>
<gate name="VE5" symbol="VDDEXT"/>
<gate name="VE6" symbol="VDDEXT"/>
<gate name="VE7" symbol="VDDEXT"/>
<gate name="VI1" symbol="VDDINT"/>
<gate name="VI2" symbol="VDDINT"/>
<gate name="VI3" symbol="VDDINT"/>
<gate name="VI4" symbol="VDDINT"/>
<gate name="VI5" symbol="VDDINT"/>
<gate name="VI6" symbol="VDDINT"/>
<gate name="VI7" symbol="VDDINT"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="F" symbol="ADSP-21161-DATA"/>
<gate name="VE8" symbol="VDDEXT"/>
<gate name="VE9" symbol="VDDEXT"/>
<gate name="VE10" symbol="VDDEXT"/>
<gate name="VE11" symbol="VDDEXT"/>
<gate name="VE12" symbol="VDDEXT"/>
<gate name="VI8" symbol="VDDINT"/>
<gate name="VI9" symbol="VDDINT"/>
<gate name="VI10" symbol="VDDINT"/>
<gate name="VI11" symbol="VDDINT"/>
<gate name="VI12" symbol="VDDINT"/>
<gate name="VI13" symbol="VDDINT"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="VE13" symbol="VDDEXT"/>
<gate name="VI14" symbol="VDDINT"/>
<gate name="AV" symbol="AVDD"/>
<gate name="AG" symbol="AGND"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
</gates>
<devices>
<device name="" package="MBGA225">
<connects>
<connect gate="A" pin="!BMS" pad="A3"/>
<connect gate="A" pin="!BR1" pad="P8"/>
<connect gate="A" pin="!BR2" pad="N8"/>
<connect gate="A" pin="!BR3" pad="R7"/>
<connect gate="A" pin="!BR4" pad="P7"/>
<connect gate="A" pin="!BR5" pad="N7"/>
<connect gate="A" pin="!BR6" pad="M7"/>
<connect gate="A" pin="!CAS" pad="L12"/>
<connect gate="A" pin="!CS" pad="N11"/>
<connect gate="A" pin="!DMAG1" pad="M15"/>
<connect gate="A" pin="!DMAG2" pad="M14"/>
<connect gate="A" pin="!DMAR1" pad="N15"/>
<connect gate="A" pin="!DMAR2" pad="P15"/>
<connect gate="A" pin="!EMU" pad="C2"/>
<connect gate="A" pin="!HBG" pad="R11"/>
<connect gate="A" pin="!HBR" pad="R10"/>
<connect gate="A" pin="!MS0" pad="N6"/>
<connect gate="A" pin="!MS1" pad="M6"/>
<connect gate="A" pin="!MS2" pad="P5"/>
<connect gate="A" pin="!MS3" pad="R5"/>
<connect gate="A" pin="!PA" pad="R6"/>
<connect gate="A" pin="!RAS" pad="M11"/>
<connect gate="A" pin="!RD" pad="R8"/>
<connect gate="A" pin="!RESET" pad="E2"/>
<connect gate="A" pin="!RSTOUT" pad="B15"/>
<connect gate="A" pin="!SBTS" pad="P6"/>
<connect gate="A" pin="!SDWE" pad="R14"/>
<connect gate="A" pin="!TRST" pad="B1"/>
<connect gate="A" pin="!WR" pad="M9"/>
<connect gate="A" pin="ACK" pad="M12"/>
<connect gate="A" pin="BMSTR" pad="A2"/>
<connect gate="A" pin="BRST" pad="N9"/>
<connect gate="A" pin="CLKOUT" pad="R9"/>
<connect gate="A" pin="DQM" pad="P13"/>
<connect gate="A" pin="REDY" pad="P11"/>
<connect gate="A" pin="SDA10" pad="M10"/>
<connect gate="A" pin="SDCKE" pad="N10"/>
<connect gate="A" pin="SDCLK0" pad="P10"/>
<connect gate="A" pin="SDCLK1" pad="P9"/>
<connect gate="A" pin="TCK" pad="D2"/>
<connect gate="A" pin="TDI" pad="B2"/>
<connect gate="A" pin="TDO" pad="D1"/>
<connect gate="A" pin="TMS" pad="C1"/>
<connect gate="AG" pin="AGND" pad="P14"/>
<connect gate="AV" pin="AVDD" pad="N14"/>
<connect gate="B" pin="!CLKDBL" pad="R12"/>
<connect gate="B" pin="!IRQ0" pad="H2"/>
<connect gate="B" pin="!IRQ1" pad="H4"/>
<connect gate="B" pin="!IRQ2" pad="J1"/>
<connect gate="B" pin="CLKIN" pad="P12"/>
<connect gate="B" pin="CLK_CFG0" pad="N13"/>
<connect gate="B" pin="CLK_CFG1" pad="N12"/>
<connect gate="B" pin="EBOOT" pad="A5"/>
<connect gate="B" pin="FLAG0" pad="H1"/>
<connect gate="B" pin="FLAG1" pad="G1"/>
<connect gate="B" pin="FLAG10" pad="E1"/>
<connect gate="B" pin="FLAG11" pad="D3"/>
<connect gate="B" pin="FLAG2" pad="G2"/>
<connect gate="B" pin="FLAG3" pad="G4"/>
<connect gate="B" pin="FLAG4" pad="G3"/>
<connect gate="B" pin="FLAG5" pad="F1"/>
<connect gate="B" pin="FLAG6" pad="F4"/>
<connect gate="B" pin="FLAG7" pad="F2"/>
<connect gate="B" pin="FLAG8" pad="E3"/>
<connect gate="B" pin="FLAG9" pad="F3"/>
<connect gate="B" pin="ID0" pad="J4"/>
<connect gate="B" pin="ID1" pad="J2"/>
<connect gate="B" pin="ID2" pad="J3"/>
<connect gate="B" pin="LBOOT" pad="A6"/>
<connect gate="B" pin="RPBA" pad="B3"/>
<connect gate="B" pin="TIMEXP" pad="K1"/>
<connect gate="B" pin="XTAL" pad="R13"/>
<connect gate="C" pin="L0ACK" pad="A10"/>
<connect gate="C" pin="L0CLK" pad="B10"/>
<connect gate="C" pin="L0DAT0" pad="E12"/>
<connect gate="C" pin="L0DAT1" pad="B11"/>
<connect gate="C" pin="L0DAT2" pad="A11"/>
<connect gate="C" pin="L0DAT3" pad="D11"/>
<connect gate="C" pin="L0DAT4" pad="A9"/>
<connect gate="C" pin="L0DAT5" pad="D10"/>
<connect gate="C" pin="L0DAT6" pad="C10"/>
<connect gate="C" pin="L0DAT7" pad="B9"/>
<connect gate="C" pin="L1ACK" pad="B13"/>
<connect gate="C" pin="L1CLK" pad="A13"/>
<connect gate="C" pin="L1DAT0" pad="B14"/>
<connect gate="C" pin="L1DAT1" pad="C13"/>
<connect gate="C" pin="L1DAT2" pad="A14"/>
<connect gate="C" pin="L1DAT3" pad="C12"/>
<connect gate="C" pin="L1DAT4" pad="B12"/>
<connect gate="C" pin="L1DAT5" pad="D12"/>
<connect gate="C" pin="L1DAT6" pad="A12"/>
<connect gate="C" pin="L1DAT7" pad="C11"/>
<connect gate="D" pin="!SPIDS" pad="A4"/>
<connect gate="D" pin="D0A" pad="E4"/>
<connect gate="D" pin="D0B" pad="C5"/>
<connect gate="D" pin="D1A" pad="C6"/>
<connect gate="D" pin="D1B" pad="D6"/>
<connect gate="D" pin="D2A" pad="C7"/>
<connect gate="D" pin="D2B" pad="B7"/>
<connect gate="D" pin="D3A" pad="B8"/>
<connect gate="D" pin="D3B" pad="A8"/>
<connect gate="D" pin="FS0" pad="B5"/>
<connect gate="D" pin="FS1" pad="D7"/>
<connect gate="D" pin="FS2" pad="C8"/>
<connect gate="D" pin="FS3" pad="C9"/>
<connect gate="D" pin="MISO" pad="D4"/>
<connect gate="D" pin="MOSI" pad="B4"/>
<connect gate="D" pin="SCLK0" pad="D5"/>
<connect gate="D" pin="SCLK1" pad="B6"/>
<connect gate="D" pin="SCLK2" pad="A7"/>
<connect gate="D" pin="SCLK3" pad="D9"/>
<connect gate="D" pin="SPICLK" pad="C4"/>
<connect gate="E" pin="AD0" pad="M5"/>
<connect gate="E" pin="AD1" pad="N5"/>
<connect gate="E" pin="AD10" pad="N3"/>
<connect gate="E" pin="AD11" pad="R2"/>
<connect gate="E" pin="AD12" pad="M2"/>
<connect gate="E" pin="AD13" pad="P1"/>
<connect gate="E" pin="AD14" pad="N1"/>
<connect gate="E" pin="AD15" pad="N2"/>
<connect gate="E" pin="AD16" pad="M1"/>
<connect gate="E" pin="AD17" pad="L2"/>
<connect gate="E" pin="AD18" pad="M3"/>
<connect gate="E" pin="AD19" pad="L1"/>
<connect gate="E" pin="AD2" pad="L4"/>
<connect gate="E" pin="AD20" pad="K3"/>
<connect gate="E" pin="AD21" pad="L3"/>
<connect gate="E" pin="AD22" pad="K2"/>
<connect gate="E" pin="AD23" pad="K4"/>
<connect gate="E" pin="AD3" pad="R4"/>
<connect gate="E" pin="AD4" pad="P4"/>
<connect gate="E" pin="AD5" pad="N4"/>
<connect gate="E" pin="AD6" pad="M4"/>
<connect gate="E" pin="AD7" pad="R3"/>
<connect gate="E" pin="AD8" pad="P3"/>
<connect gate="E" pin="AD9" pad="P2"/>
<connect gate="F" pin="D16" pad="L14"/>
<connect gate="F" pin="D17" pad="M13"/>
<connect gate="F" pin="D18" pad="L15"/>
<connect gate="F" pin="D19" pad="K13"/>
<connect gate="F" pin="D20" pad="L13"/>
<connect gate="F" pin="D21" pad="K14"/>
<connect gate="F" pin="D22" pad="K12"/>
<connect gate="F" pin="D23" pad="K15"/>
<connect gate="F" pin="D24" pad="J13"/>
<connect gate="F" pin="D25" pad="J14"/>
<connect gate="F" pin="D26" pad="J12"/>
<connect gate="F" pin="D27" pad="J15"/>
<connect gate="F" pin="D28" pad="H13"/>
<connect gate="F" pin="D29" pad="H12"/>
<connect gate="F" pin="D30" pad="H14"/>
<connect gate="F" pin="D31" pad="H15"/>
<connect gate="F" pin="D32" pad="G15"/>
<connect gate="F" pin="D33" pad="G14"/>
<connect gate="F" pin="D34" pad="G12"/>
<connect gate="F" pin="D35" pad="G13"/>
<connect gate="F" pin="D36" pad="F15"/>
<connect gate="F" pin="D37" pad="F12"/>
<connect gate="F" pin="D38" pad="F14"/>
<connect gate="F" pin="D39" pad="E13"/>
<connect gate="F" pin="D40" pad="F13"/>
<connect gate="F" pin="D41" pad="E15"/>
<connect gate="F" pin="D42" pad="D13"/>
<connect gate="F" pin="D43" pad="E14"/>
<connect gate="F" pin="D44" pad="D15"/>
<connect gate="F" pin="D45" pad="C14"/>
<connect gate="F" pin="D46" pad="D14"/>
<connect gate="F" pin="D47" pad="C15"/>
<connect gate="G1" pin="GND" pad="C3"/>
<connect gate="G10" pin="GND" pad="F6"/>
<connect gate="G11" pin="GND" pad="F7"/>
<connect gate="G12" pin="GND" pad="F8"/>
<connect gate="G13" pin="GND" pad="F9"/>
<connect gate="G14" pin="GND" pad="F10"/>
<connect gate="G15" pin="GND" pad="H9"/>
<connect gate="G16" pin="GND" pad="H10"/>
<connect gate="G17" pin="GND" pad="J6"/>
<connect gate="G18" pin="GND" pad="J7"/>
<connect gate="G19" pin="GND" pad="J8"/>
<connect gate="G2" pin="GND" pad="G6"/>
<connect gate="G20" pin="GND" pad="J9"/>
<connect gate="G21" pin="GND" pad="J10"/>
<connect gate="G22" pin="GND" pad="K6"/>
<connect gate="G23" pin="GND" pad="K7"/>
<connect gate="G24" pin="GND" pad="K8"/>
<connect gate="G25" pin="GND" pad="K9"/>
<connect gate="G26" pin="GND" pad="K10"/>
<connect gate="G3" pin="GND" pad="G7"/>
<connect gate="G4" pin="GND" pad="G8"/>
<connect gate="G5" pin="GND" pad="G9"/>
<connect gate="G6" pin="GND" pad="G10"/>
<connect gate="G7" pin="GND" pad="H6"/>
<connect gate="G8" pin="GND" pad="H7"/>
<connect gate="G9" pin="GND" pad="H8"/>
<connect gate="NC1" pin="NC" pad="A1"/>
<connect gate="NC2" pin="NC" pad="A15"/>
<connect gate="NC3" pin="NC" pad="R1"/>
<connect gate="NC4" pin="NC" pad="R15"/>
<connect gate="VE1" pin="VDDEXT" pad="E5"/>
<connect gate="VE10" pin="VDDEXT" pad="L7"/>
<connect gate="VE11" pin="VDDEXT" pad="L9"/>
<connect gate="VE12" pin="VDDEXT" pad="L11"/>
<connect gate="VE13" pin="VDDEXT" pad="M8"/>
<connect gate="VE2" pin="VDDEXT" pad="E7"/>
<connect gate="VE3" pin="VDDEXT" pad="E9"/>
<connect gate="VE4" pin="VDDEXT" pad="E11"/>
<connect gate="VE5" pin="VDDEXT" pad="G5"/>
<connect gate="VE6" pin="VDDEXT" pad="G11"/>
<connect gate="VE7" pin="VDDEXT" pad="J5"/>
<connect gate="VE8" pin="VDDEXT" pad="J11"/>
<connect gate="VE9" pin="VDDEXT" pad="L5"/>
<connect gate="VI1" pin="VDDINT" pad="D8"/>
<connect gate="VI10" pin="VDDINT" pad="K5"/>
<connect gate="VI11" pin="VDDINT" pad="K11"/>
<connect gate="VI12" pin="VDDINT" pad="L6"/>
<connect gate="VI13" pin="VDDINT" pad="L8"/>
<connect gate="VI14" pin="VDDINT" pad="L10"/>
<connect gate="VI2" pin="VDDINT" pad="E6"/>
<connect gate="VI3" pin="VDDINT" pad="E8"/>
<connect gate="VI4" pin="VDDINT" pad="E10"/>
<connect gate="VI5" pin="VDDINT" pad="F5"/>
<connect gate="VI6" pin="VDDINT" pad="F11"/>
<connect gate="VI7" pin="VDDINT" pad="H3"/>
<connect gate="VI8" pin="VDDINT" pad="H5"/>
<connect gate="VI9" pin="VDDINT" pad="H11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADSP-21161NCCA-100"/>
<attribute name="OC_FARNELL" value="1465539"/>
<attribute name="OC_NEWARK" value="02H1229"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC814*" prefix="IC">
<description>&lt;b&gt;MicroConverter®&lt;/b&gt; 12-Bit ADC with Embedded FLASH MCU&lt;p&gt;
 Small Package</description>
<gates>
<gate name="G$1" symbol="ADUC814"/>
</gates>
<devices>
<device name="RU" package="TSSOP28">
<connects>
<connect gate="G$1" pin="AGND@1" pad="14"/>
<connect gate="G$1" pin="AGND@2" pad="15"/>
<connect gate="G$1" pin="AVDD" pad="13"/>
<connect gate="G$1" pin="CREF" pad="17"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="DLOAD" pad="2"/>
<connect gate="G$1" pin="DVDD" pad="28"/>
<connect gate="G$1" pin="P1.0/T2" pad="8"/>
<connect gate="G$1" pin="P1.1/T2EX" pad="9"/>
<connect gate="G$1" pin="P1.2/ADC0" pad="11"/>
<connect gate="G$1" pin="P1.3/ADC1" pad="12"/>
<connect gate="G$1" pin="P1.4/ADC2" pad="18"/>
<connect gate="G$1" pin="P1.5/ADC3" pad="19"/>
<connect gate="G$1" pin="P1.6/ADC4/DAC0" pad="20"/>
<connect gate="G$1" pin="P1.7/ADC5/DAC1" pad="21"/>
<connect gate="G$1" pin="P3.0/RXD" pad="3"/>
<connect gate="G$1" pin="P3.1/TXD" pad="4"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="5"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="6"/>
<connect gate="G$1" pin="P3.4/!CONVST" pad="7"/>
<connect gate="G$1" pin="P3.5/T1/!SS!/EXTCLK" pad="22"/>
<connect gate="G$1" pin="P3.6/MISO" pad="23"/>
<connect gate="G$1" pin="P3.7/MOSI" pad="24"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="SCLOCK" pad="25"/>
<connect gate="G$1" pin="VREF" pad="16"/>
<connect gate="G$1" pin="XTAL1" pad="26"/>
<connect gate="G$1" pin="XTAL2" pad="27"/>
</connects>
<technologies>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC814ARUZ"/>
<attribute name="OC_FARNELL" value="9426361"/>
<attribute name="OC_NEWARK" value="31M3924"/>
</technology>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC814BRU"/>
<attribute name="OC_FARNELL" value="1424536"/>
<attribute name="OC_NEWARK" value="92C2265"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8133" prefix="IC">
<description>&lt;b&gt;Triple Differential Driver&lt;/b&gt; With Output Pull-Down&lt;p&gt;
Source: http://www.analog.com .. 3832984220209AD8133_0.pdf</description>
<gates>
<gate name="G$1" symbol="AD8133"/>
</gates>
<devices>
<device name="" package="LFCSP24">
<connects>
<connect gate="G$1" pin="+INA" pad="4"/>
<connect gate="G$1" pin="+INB" pad="23"/>
<connect gate="G$1" pin="+INC" pad="15"/>
<connect gate="G$1" pin="+OUTA" pad="7"/>
<connect gate="G$1" pin="+OUTB" pad="9"/>
<connect gate="G$1" pin="+OUTC" pad="12"/>
<connect gate="G$1" pin="-INA" pad="3"/>
<connect gate="G$1" pin="-INB" pad="22"/>
<connect gate="G$1" pin="-INC" pad="16"/>
<connect gate="G$1" pin="-OUTA" pad="6"/>
<connect gate="G$1" pin="-OUTB" pad="10"/>
<connect gate="G$1" pin="-OUTC" pad="13"/>
<connect gate="G$1" pin="OPD" pad="1"/>
<connect gate="G$1" pin="VCOMA" pad="20"/>
<connect gate="G$1" pin="VCOMB" pad="19"/>
<connect gate="G$1" pin="VCOMC" pad="18"/>
<connect gate="G$1" pin="VS+@1" pad="8"/>
<connect gate="G$1" pin="VS+@2" pad="11"/>
<connect gate="G$1" pin="VS+@3" pad="17"/>
<connect gate="G$1" pin="VS+@4" pad="24"/>
<connect gate="G$1" pin="VS-@1" pad="2"/>
<connect gate="G$1" pin="VS-@2" pad="5"/>
<connect gate="G$1" pin="VS-@3" pad="14"/>
<connect gate="G$1" pin="VS-@4" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8133ACPZ-REEL7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K6409"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADXL202E" prefix="IC">
<description>&lt;b&gt;Low-Cost  +-2 g Dual-Axis Accelerometer&lt;/b&gt; with Duty Cycle Output&lt;p&gt;
Source: www.analog.com/UploadedFiles/Data_Sheets/53728567227477ADXL202E_a.pdf</description>
<gates>
<gate name="G$1" symbol="ADXL202"/>
</gates>
<devices>
<device name="" package="LCC8">
<connects>
<connect gate="G$1" pin="COM" pad="3"/>
<connect gate="G$1" pin="ST" pad="1"/>
<connect gate="G$1" pin="T2" pad="2"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="XFILT" pad="7"/>
<connect gate="G$1" pin="XOUT" pad="5"/>
<connect gate="G$1" pin="YFILT" pad="6"/>
<connect gate="G$1" pin="YOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADXL202JE"/>
<attribute name="OC_FARNELL" value="1424583"/>
<attribute name="OC_NEWARK" value="23C7726"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD650" prefix="IC">
<description>&lt;b&gt;AD650 - Voltage-to-Frequency and Frequency-to-Voltage Converter&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/en/prod/0,,760_794_AD650,00.html</description>
<gates>
<gate name="P" symbol="AD650"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="P" pin="+IN" pad="2"/>
<connect gate="P" pin="+VS" pad="12"/>
<connect gate="P" pin="-IN" pad="3"/>
<connect gate="P" pin="-VS" pad="5"/>
<connect gate="P" pin="AGND" pad="11"/>
<connect gate="P" pin="BOC" pad="4"/>
<connect gate="P" pin="COMP_IN" pad="9"/>
<connect gate="P" pin="DGND" pad="10"/>
<connect gate="P" pin="FOUT" pad="8"/>
<connect gate="P" pin="OFF0" pad="13"/>
<connect gate="P" pin="OFF1" pad="14"/>
<connect gate="P" pin="ONESHOT" pad="6"/>
<connect gate="P" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD650KN"/>
<attribute name="OC_FARNELL" value="1464457"/>
<attribute name="OC_NEWARK" value="05F7159"/>
</technology>
</technologies>
</device>
<device name="P" package="PLCC20">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="+VS" pad="18"/>
<connect gate="P" pin="-IN" pad="4"/>
<connect gate="P" pin="-VS" pad="8"/>
<connect gate="P" pin="AGND" pad="16"/>
<connect gate="P" pin="BOC" pad="6"/>
<connect gate="P" pin="COMP_IN" pad="13"/>
<connect gate="P" pin="DGND" pad="14"/>
<connect gate="P" pin="FOUT" pad="12"/>
<connect gate="P" pin="OFF0" pad="19"/>
<connect gate="P" pin="OFF1" pad="20"/>
<connect gate="P" pin="ONESHOT" pad="9"/>
<connect gate="P" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7568" prefix="IC">
<description>&lt;b&gt;LC2MOS Octal 12-Bit DAC&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/843987253ad7568.pdf</description>
<gates>
<gate name="G$1" symbol="AD7568"/>
</gates>
<devices>
<device name="S" package="PQFP44">
<connects>
<connect gate="G$1" pin="!CLR" pad="15"/>
<connect gate="G$1" pin="!FSIN" pad="17"/>
<connect gate="G$1" pin="!LDAG" pad="16"/>
<connect gate="G$1" pin="A0" pad="20"/>
<connect gate="G$1" pin="AGND" pad="38"/>
<connect gate="G$1" pin="CLKIN" pad="19"/>
<connect gate="G$1" pin="DGND" pad="39"/>
<connect gate="G$1" pin="IOUT1A" pad="22"/>
<connect gate="G$1" pin="IOUT1B" pad="26"/>
<connect gate="G$1" pin="IOUT1C" pad="30"/>
<connect gate="G$1" pin="IOUT1D" pad="35"/>
<connect gate="G$1" pin="IOUT1E" pad="43"/>
<connect gate="G$1" pin="IOUT1F" pad="4"/>
<connect gate="G$1" pin="IOUT1G" pad="8"/>
<connect gate="G$1" pin="IOUT1H" pad="12"/>
<connect gate="G$1" pin="IOUT2A" pad="21"/>
<connect gate="G$1" pin="IOUT2B" pad="25"/>
<connect gate="G$1" pin="IOUT2C" pad="29"/>
<connect gate="G$1" pin="IOUT2D" pad="34"/>
<connect gate="G$1" pin="IOUT2E" pad="44"/>
<connect gate="G$1" pin="IOUT2F" pad="5"/>
<connect gate="G$1" pin="IOUT2G" pad="9"/>
<connect gate="G$1" pin="IOUT2H" pad="13"/>
<connect gate="G$1" pin="RFBA" pad="23"/>
<connect gate="G$1" pin="RFBB" pad="42"/>
<connect gate="G$1" pin="RFBC" pad="31"/>
<connect gate="G$1" pin="RFBD" pad="36"/>
<connect gate="G$1" pin="RFBE" pad="27"/>
<connect gate="G$1" pin="RFBF" pad="3"/>
<connect gate="G$1" pin="RFBG" pad="7"/>
<connect gate="G$1" pin="RFBH" pad="11"/>
<connect gate="G$1" pin="SDIN" pad="18"/>
<connect gate="G$1" pin="SDOUT" pad="14"/>
<connect gate="G$1" pin="VDD" pad="40"/>
<connect gate="G$1" pin="VREFA" pad="24"/>
<connect gate="G$1" pin="VREFB" pad="28"/>
<connect gate="G$1" pin="VREFC" pad="32"/>
<connect gate="G$1" pin="VREFD" pad="37"/>
<connect gate="G$1" pin="VREFE" pad="41"/>
<connect gate="G$1" pin="VREFF" pad="2"/>
<connect gate="G$1" pin="VREFG" pad="6"/>
<connect gate="G$1" pin="VREFH" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7568BSZ"/>
<attribute name="OC_FARNELL" value="1311330"/>
<attribute name="OC_NEWARK" value="59K5056"/>
</technology>
</technologies>
</device>
<device name="P" package="PLCC44">
<connects>
<connect gate="G$1" pin="!CLR" pad="21"/>
<connect gate="G$1" pin="!FSIN" pad="23"/>
<connect gate="G$1" pin="!LDAG" pad="22"/>
<connect gate="G$1" pin="A0" pad="26"/>
<connect gate="G$1" pin="AGND" pad="44"/>
<connect gate="G$1" pin="CLKIN" pad="25"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="IOUT1A" pad="28"/>
<connect gate="G$1" pin="IOUT1B" pad="32"/>
<connect gate="G$1" pin="IOUT1C" pad="36"/>
<connect gate="G$1" pin="IOUT1D" pad="41"/>
<connect gate="G$1" pin="IOUT1E" pad="5"/>
<connect gate="G$1" pin="IOUT1F" pad="10"/>
<connect gate="G$1" pin="IOUT1G" pad="14"/>
<connect gate="G$1" pin="IOUT1H" pad="18"/>
<connect gate="G$1" pin="IOUT2A" pad="27"/>
<connect gate="G$1" pin="IOUT2B" pad="31"/>
<connect gate="G$1" pin="IOUT2C" pad="35"/>
<connect gate="G$1" pin="IOUT2D" pad="40"/>
<connect gate="G$1" pin="IOUT2E" pad="6"/>
<connect gate="G$1" pin="IOUT2F" pad="11"/>
<connect gate="G$1" pin="IOUT2G" pad="15"/>
<connect gate="G$1" pin="IOUT2H" pad="19"/>
<connect gate="G$1" pin="RFBA" pad="29"/>
<connect gate="G$1" pin="RFBB" pad="33"/>
<connect gate="G$1" pin="RFBC" pad="37"/>
<connect gate="G$1" pin="RFBD" pad="42"/>
<connect gate="G$1" pin="RFBE" pad="4"/>
<connect gate="G$1" pin="RFBF" pad="9"/>
<connect gate="G$1" pin="RFBG" pad="13"/>
<connect gate="G$1" pin="RFBH" pad="17"/>
<connect gate="G$1" pin="SDIN" pad="24"/>
<connect gate="G$1" pin="SDOUT" pad="20"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VREFA" pad="30"/>
<connect gate="G$1" pin="VREFB" pad="34"/>
<connect gate="G$1" pin="VREFC" pad="38"/>
<connect gate="G$1" pin="VREFD" pad="43"/>
<connect gate="G$1" pin="VREFE" pad="3"/>
<connect gate="G$1" pin="VREFF" pad="8"/>
<connect gate="G$1" pin="VREFG" pad="12"/>
<connect gate="G$1" pin="VREFH" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD7568BP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="09B5836"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7524*" prefix="IC">
<description>&lt;b&gt;8-Bit Buffered Multiplying DAC&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/888358036ad7524.pdf</description>
<gates>
<gate name="G$1" symbol="AD7524"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="!CS" pad="12"/>
<connect gate="G$1" pin="!WR" pad="13"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="D5" pad="6"/>
<connect gate="G$1" pin="D6" pad="5"/>
<connect gate="G$1" pin="D7" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name="J">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524JNZ"/>
<attribute name="OC_FARNELL" value="9605401"/>
<attribute name="OC_NEWARK" value="59K4969"/>
</technology>
<technology name="K">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524KNZ"/>
<attribute name="OC_FARNELL" value="1464568"/>
<attribute name="OC_NEWARK" value="59K4973"/>
</technology>
<technology name="L">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524LNZ"/>
<attribute name="OC_FARNELL" value="9605401"/>
<attribute name="OC_NEWARK" value="59K4974"/>
</technology>
</technologies>
</device>
<device name="R" package="SOIC16N">
<connects>
<connect gate="G$1" pin="!CS" pad="12"/>
<connect gate="G$1" pin="!WR" pad="13"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="D5" pad="6"/>
<connect gate="G$1" pin="D6" pad="5"/>
<connect gate="G$1" pin="D7" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name="J">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524JRZ"/>
<attribute name="OC_FARNELL" value="1423882"/>
<attribute name="OC_NEWARK" value="59K4970"/>
</technology>
</technologies>
</device>
<device name="P" package="PLCC20">
<connects>
<connect gate="G$1" pin="!CS" pad="15"/>
<connect gate="G$1" pin="!WR" pad="17"/>
<connect gate="G$1" pin="D0" pad="14"/>
<connect gate="G$1" pin="D1" pad="13"/>
<connect gate="G$1" pin="D2" pad="12"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="9"/>
<connect gate="G$1" pin="D5" pad="8"/>
<connect gate="G$1" pin="D6" pad="7"/>
<connect gate="G$1" pin="D7" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="RFB" pad="20"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VREF" pad="19"/>
</connects>
<technologies>
<technology name="J">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524JP"/>
<attribute name="OC_FARNELL" value="1464569"/>
<attribute name="OC_NEWARK" value="05F7382"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1464569"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524LP"/>
<attribute name="OC_FARNELL" value="1464569"/>
<attribute name="OC_NEWARK" value="09B5765"/>
</technology>
</technologies>
</device>
<device name="E" package="LCC20">
<connects>
<connect gate="G$1" pin="!CS" pad="15"/>
<connect gate="G$1" pin="!WR" pad="17"/>
<connect gate="G$1" pin="D0" pad="14"/>
<connect gate="G$1" pin="D1" pad="13"/>
<connect gate="G$1" pin="D2" pad="12"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="9"/>
<connect gate="G$1" pin="D5" pad="8"/>
<connect gate="G$1" pin="D6" pad="7"/>
<connect gate="G$1" pin="D7" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="2"/>
<connect gate="G$1" pin="OUT2" pad="3"/>
<connect gate="G$1" pin="RFB" pad="20"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VREF" pad="19"/>
</connects>
<technologies>
<technology name="S">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524JP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="05F7382"/>
</technology>
<technology name="T">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524JP"/>
<attribute name="OC_FARNELL" value="1464569"/>
<attribute name="OC_NEWARK" value="05F7382"/>
</technology>
<technology name="U">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524KP"/>
<attribute name="OC_FARNELL" value="1464569"/>
<attribute name="OC_NEWARK" value="09B5764"/>
</technology>
</technologies>
</device>
<device name="Q" package="DIL16">
<connects>
<connect gate="G$1" pin="!CS" pad="12"/>
<connect gate="G$1" pin="!WR" pad="13"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="D5" pad="6"/>
<connect gate="G$1" pin="D6" pad="5"/>
<connect gate="G$1" pin="D7" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="2"/>
<connect gate="G$1" pin="RFB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name="A">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524AQ"/>
<attribute name="OC_FARNELL" value="1464568"/>
<attribute name="OC_NEWARK" value="05F7379"/>
</technology>
<technology name="B">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524KP"/>
<attribute name="OC_FARNELL" value="9605401"/>
<attribute name="OC_NEWARK" value="09B5764"/>
</technology>
<technology name="C">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524TQ"/>
<attribute name="OC_FARNELL" value="1523901"/>
<attribute name="OC_NEWARK" value="16F3371"/>
</technology>
<technology name="S">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524SQ"/>
<attribute name="OC_FARNELL" value="9605401"/>
<attribute name="OC_NEWARK" value="16F3370"/>
</technology>
<technology name="T">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524TQ"/>
<attribute name="OC_FARNELL" value="9605401"/>
<attribute name="OC_NEWARK" value="16F3371"/>
</technology>
<technology name="U">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7524SQ"/>
<attribute name="OC_FARNELL" value="1523901"/>
<attribute name="OC_NEWARK" value="16F3370"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_BF533" prefix="IC">
<description>&lt;b&gt;ADSP-BF533 - Blackfin Processor for Video/Imaging&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp&lt;/i&gt;&lt;br&gt;
Source: 33260205658992ADSP_BF533_mbga.bsdl</description>
<gates>
<gate name="G$1" symbol="ADSP_BF533_MBGA"/>
</gates>
<devices>
<device name="" package="MBGA_160">
<connects>
<connect gate="G$1" pin="ABE_B0" pad="H13"/>
<connect gate="G$1" pin="ABE_B1" pad="H12"/>
<connect gate="G$1" pin="ADDR1" pad="J14"/>
<connect gate="G$1" pin="ADDR10" pad="M13"/>
<connect gate="G$1" pin="ADDR11" pad="M14"/>
<connect gate="G$1" pin="ADDR12" pad="N14"/>
<connect gate="G$1" pin="ADDR13" pad="N13"/>
<connect gate="G$1" pin="ADDR14" pad="N12"/>
<connect gate="G$1" pin="ADDR15" pad="M11"/>
<connect gate="G$1" pin="ADDR16" pad="N11"/>
<connect gate="G$1" pin="ADDR17" pad="P13"/>
<connect gate="G$1" pin="ADDR18" pad="P12"/>
<connect gate="G$1" pin="ADDR19" pad="P11"/>
<connect gate="G$1" pin="ADDR2" pad="K14"/>
<connect gate="G$1" pin="ADDR3" pad="L14"/>
<connect gate="G$1" pin="ADDR4" pad="J13"/>
<connect gate="G$1" pin="ADDR5" pad="K13"/>
<connect gate="G$1" pin="ADDR6" pad="L13"/>
<connect gate="G$1" pin="ADDR7" pad="K12"/>
<connect gate="G$1" pin="ADDR8" pad="L12"/>
<connect gate="G$1" pin="ADDR9" pad="M12"/>
<connect gate="G$1" pin="AMS_B0" pad="E14"/>
<connect gate="G$1" pin="AMS_B1" pad="F14"/>
<connect gate="G$1" pin="AMS_B2" pad="F13"/>
<connect gate="G$1" pin="AMS_B3" pad="G12"/>
<connect gate="G$1" pin="AOE_B" pad="G13"/>
<connect gate="G$1" pin="ARDY" pad="E13"/>
<connect gate="G$1" pin="ARE_B" pad="G14"/>
<connect gate="G$1" pin="AWE_B" pad="H14"/>
<connect gate="G$1" pin="BGH_B" pad="N10"/>
<connect gate="G$1" pin="BG_B" pad="P10"/>
<connect gate="G$1" pin="BMODE0" pad="N4"/>
<connect gate="G$1" pin="BMODE1" pad="P3"/>
<connect gate="G$1" pin="BR_B" pad="D14"/>
<connect gate="G$1" pin="CLKIN" pad="A12"/>
<connect gate="G$1" pin="CLKOUT" pad="B14"/>
<connect gate="G$1" pin="DATA0" pad="M9"/>
<connect gate="G$1" pin="DATA1" pad="N9"/>
<connect gate="G$1" pin="DATA10" pad="N6"/>
<connect gate="G$1" pin="DATA11" pad="P6"/>
<connect gate="G$1" pin="DATA12" pad="M5"/>
<connect gate="G$1" pin="DATA13" pad="N5"/>
<connect gate="G$1" pin="DATA14" pad="P5"/>
<connect gate="G$1" pin="DATA15" pad="P4"/>
<connect gate="G$1" pin="DATA2" pad="P9"/>
<connect gate="G$1" pin="DATA3" pad="M8"/>
<connect gate="G$1" pin="DATA4" pad="N8"/>
<connect gate="G$1" pin="DATA5" pad="P8"/>
<connect gate="G$1" pin="DATA6" pad="M7"/>
<connect gate="G$1" pin="DATA7" pad="N7"/>
<connect gate="G$1" pin="DATA8" pad="P7"/>
<connect gate="G$1" pin="DATA9" pad="M6"/>
<connect gate="G$1" pin="DR0PRI" pad="K1"/>
<connect gate="G$1" pin="DR0SEC" pad="J2"/>
<connect gate="G$1" pin="DR1PRI" pad="G3"/>
<connect gate="G$1" pin="DR1SEC" pad="F3"/>
<connect gate="G$1" pin="DT0PRI" pad="H1"/>
<connect gate="G$1" pin="DT0SEC" pad="H2"/>
<connect gate="G$1" pin="DT1PRI" pad="F2"/>
<connect gate="G$1" pin="DT1SEC" pad="E3"/>
<connect gate="G$1" pin="EMU_B" pad="M2"/>
<connect gate="G$1" pin="GND@0" pad="H4"/>
<connect gate="G$1" pin="GND@1" pad="A14"/>
<connect gate="G$1" pin="GND@10" pad="L5"/>
<connect gate="G$1" pin="GND@11" pad="P14"/>
<connect gate="G$1" pin="GND@12" pad="C4"/>
<connect gate="G$1" pin="GND@13" pad="D10"/>
<connect gate="G$1" pin="GND@14" pad="L6"/>
<connect gate="G$1" pin="GND@15" pad="C5"/>
<connect gate="G$1" pin="GND@16" pad="D7"/>
<connect gate="G$1" pin="GND@17" pad="F11"/>
<connect gate="G$1" pin="GND@18" pad="D4"/>
<connect gate="G$1" pin="GND@19" pad="K4"/>
<connect gate="G$1" pin="GND@2" pad="D11"/>
<connect gate="G$1" pin="GND@20" pad="K11"/>
<connect gate="G$1" pin="GND@21" pad="L8"/>
<connect gate="G$1" pin="GND@22" pad="A10"/>
<connect gate="G$1" pin="GND@23" pad="B11"/>
<connect gate="G$1" pin="GND@3" pad="L10"/>
<connect gate="G$1" pin="GND@4" pad="C11"/>
<connect gate="G$1" pin="GND@5" pad="H11"/>
<connect gate="G$1" pin="GND@6" pad="F4"/>
<connect gate="G$1" pin="GND@7" pad="G11"/>
<connect gate="G$1" pin="GND@8" pad="M10"/>
<connect gate="G$1" pin="GND@9" pad="D8"/>
<connect gate="G$1" pin="MISO" pad="E2"/>
<connect gate="G$1" pin="MOSI" pad="D3"/>
<connect gate="G$1" pin="NMI" pad="B10"/>
<connect gate="G$1" pin="PF0" pad="D2"/>
<connect gate="G$1" pin="PF1" pad="C1"/>
<connect gate="G$1" pin="PF10" pad="A4"/>
<connect gate="G$1" pin="PF11" pad="A5"/>
<connect gate="G$1" pin="PF12" pad="B5"/>
<connect gate="G$1" pin="PF13" pad="B6"/>
<connect gate="G$1" pin="PF14" pad="A6"/>
<connect gate="G$1" pin="PF15" pad="C6"/>
<connect gate="G$1" pin="PF2" pad="C2"/>
<connect gate="G$1" pin="PF3" pad="C3"/>
<connect gate="G$1" pin="PF4" pad="B1"/>
<connect gate="G$1" pin="PF5" pad="B2"/>
<connect gate="G$1" pin="PF6" pad="B3"/>
<connect gate="G$1" pin="PF7" pad="B4"/>
<connect gate="G$1" pin="PF8" pad="A2"/>
<connect gate="G$1" pin="PF9" pad="A3"/>
<connect gate="G$1" pin="PP0" pad="C8"/>
<connect gate="G$1" pin="PP1" pad="B8"/>
<connect gate="G$1" pin="PP2" pad="A7"/>
<connect gate="G$1" pin="PP3" pad="B7"/>
<connect gate="G$1" pin="PP_CLK" pad="C9"/>
<connect gate="G$1" pin="RESET_B" pad="C10"/>
<connect gate="G$1" pin="RFS0" pad="J3"/>
<connect gate="G$1" pin="RFS1" pad="G2"/>
<connect gate="G$1" pin="RSCLK0" pad="L1"/>
<connect gate="G$1" pin="RSCLK1" pad="G1"/>
<connect gate="G$1" pin="RTXI" pad="A9"/>
<connect gate="G$1" pin="RTXO" pad="A8"/>
<connect gate="G$1" pin="RX" pad="L3"/>
<connect gate="G$1" pin="SA10" pad="E12"/>
<connect gate="G$1" pin="SCAS_B" pad="C14"/>
<connect gate="G$1" pin="SCK" pad="D1"/>
<connect gate="G$1" pin="SCKE" pad="B13"/>
<connect gate="G$1" pin="SMS_B" pad="C13"/>
<connect gate="G$1" pin="SRAS_B" pad="D13"/>
<connect gate="G$1" pin="SWE_B" pad="D12"/>
<connect gate="G$1" pin="TCK" pad="P2"/>
<connect gate="G$1" pin="TDI" pad="M3"/>
<connect gate="G$1" pin="TDO" pad="N3"/>
<connect gate="G$1" pin="TEST" pad="M4"/>
<connect gate="G$1" pin="TFS0" pad="H3"/>
<connect gate="G$1" pin="TFS1" pad="E1"/>
<connect gate="G$1" pin="TMR0" pad="L2"/>
<connect gate="G$1" pin="TMR1" pad="M1"/>
<connect gate="G$1" pin="TMR2" pad="K2"/>
<connect gate="G$1" pin="TMS" pad="N2"/>
<connect gate="G$1" pin="TRST_B" pad="N1"/>
<connect gate="G$1" pin="TSCLK0" pad="J1"/>
<connect gate="G$1" pin="TSCLK1" pad="F1"/>
<connect gate="G$1" pin="TX" pad="K3"/>
<connect gate="G$1" pin="VDD_EXT@0" pad="J12"/>
<connect gate="G$1" pin="VDD_EXT@1" pad="F12"/>
<connect gate="G$1" pin="VDD_EXT@10" pad="G4"/>
<connect gate="G$1" pin="VDD_EXT@11" pad="C12"/>
<connect gate="G$1" pin="VDD_EXT@2" pad="C7"/>
<connect gate="G$1" pin="VDD_EXT@3" pad="A1"/>
<connect gate="G$1" pin="VDD_EXT@4" pad="P1"/>
<connect gate="G$1" pin="VDD_EXT@5" pad="J4"/>
<connect gate="G$1" pin="VDD_EXT@6" pad="D9"/>
<connect gate="G$1" pin="VDD_EXT@7" pad="L11"/>
<connect gate="G$1" pin="VDD_EXT@8" pad="L7"/>
<connect gate="G$1" pin="VDD_EXT@9" pad="D5"/>
<connect gate="G$1" pin="VDD_INT@0" pad="J11"/>
<connect gate="G$1" pin="VDD_INT@1" pad="D6"/>
<connect gate="G$1" pin="VDD_INT@2" pad="E4"/>
<connect gate="G$1" pin="VDD_INT@3" pad="E11"/>
<connect gate="G$1" pin="VDD_INT@4" pad="L9"/>
<connect gate="G$1" pin="VDD_INT@5" pad="L4"/>
<connect gate="G$1" pin="VDD_RTC" pad="B9"/>
<connect gate="G$1" pin="VROUT@0" pad="A13"/>
<connect gate="G$1" pin="VROUT@1" pad="B12"/>
<connect gate="G$1" pin="XTAL" pad="A11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1465585"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_BF531" prefix="IC">
<description>&lt;b&gt;ADSP BF531&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 8&lt;/i&gt;&lt;br&gt;
Source: 33170285923617ADSP_BF531_mbga.bsdl</description>
<gates>
<gate name="G$1" symbol="33170285923617ADSP_BF531_MBGA"/>
</gates>
<devices>
<device name="" package="MBGA_160">
<connects>
<connect gate="G$1" pin="ABE_B0" pad="H13"/>
<connect gate="G$1" pin="ABE_B1" pad="H12"/>
<connect gate="G$1" pin="ADDR1" pad="J14"/>
<connect gate="G$1" pin="ADDR10" pad="M13"/>
<connect gate="G$1" pin="ADDR11" pad="M14"/>
<connect gate="G$1" pin="ADDR12" pad="N14"/>
<connect gate="G$1" pin="ADDR13" pad="N13"/>
<connect gate="G$1" pin="ADDR14" pad="N12"/>
<connect gate="G$1" pin="ADDR15" pad="M11"/>
<connect gate="G$1" pin="ADDR16" pad="N11"/>
<connect gate="G$1" pin="ADDR17" pad="P13"/>
<connect gate="G$1" pin="ADDR18" pad="P12"/>
<connect gate="G$1" pin="ADDR19" pad="P11"/>
<connect gate="G$1" pin="ADDR2" pad="K14"/>
<connect gate="G$1" pin="ADDR3" pad="L14"/>
<connect gate="G$1" pin="ADDR4" pad="J13"/>
<connect gate="G$1" pin="ADDR5" pad="K13"/>
<connect gate="G$1" pin="ADDR6" pad="L13"/>
<connect gate="G$1" pin="ADDR7" pad="K12"/>
<connect gate="G$1" pin="ADDR8" pad="L12"/>
<connect gate="G$1" pin="ADDR9" pad="M12"/>
<connect gate="G$1" pin="AMS_B0" pad="E14"/>
<connect gate="G$1" pin="AMS_B1" pad="F14"/>
<connect gate="G$1" pin="AMS_B2" pad="F13"/>
<connect gate="G$1" pin="AMS_B3" pad="G12"/>
<connect gate="G$1" pin="AOE_B" pad="G13"/>
<connect gate="G$1" pin="ARDY" pad="E13"/>
<connect gate="G$1" pin="ARE_B" pad="G14"/>
<connect gate="G$1" pin="AWE_B" pad="H14"/>
<connect gate="G$1" pin="BGH_B" pad="N10"/>
<connect gate="G$1" pin="BG_B" pad="P10"/>
<connect gate="G$1" pin="BMODE0" pad="N4"/>
<connect gate="G$1" pin="BMODE1" pad="P3"/>
<connect gate="G$1" pin="BR_B" pad="D14"/>
<connect gate="G$1" pin="CLKIN" pad="A12"/>
<connect gate="G$1" pin="CLKOUT" pad="B14"/>
<connect gate="G$1" pin="DATA0" pad="M9"/>
<connect gate="G$1" pin="DATA1" pad="N9"/>
<connect gate="G$1" pin="DATA10" pad="N6"/>
<connect gate="G$1" pin="DATA11" pad="P6"/>
<connect gate="G$1" pin="DATA12" pad="M5"/>
<connect gate="G$1" pin="DATA13" pad="N5"/>
<connect gate="G$1" pin="DATA14" pad="P5"/>
<connect gate="G$1" pin="DATA15" pad="P4"/>
<connect gate="G$1" pin="DATA2" pad="P9"/>
<connect gate="G$1" pin="DATA3" pad="M8"/>
<connect gate="G$1" pin="DATA4" pad="N8"/>
<connect gate="G$1" pin="DATA5" pad="P8"/>
<connect gate="G$1" pin="DATA6" pad="M7"/>
<connect gate="G$1" pin="DATA7" pad="N7"/>
<connect gate="G$1" pin="DATA8" pad="P7"/>
<connect gate="G$1" pin="DATA9" pad="M6"/>
<connect gate="G$1" pin="DR0PRI" pad="K1"/>
<connect gate="G$1" pin="DR0SEC" pad="J2"/>
<connect gate="G$1" pin="DR1PRI" pad="G3"/>
<connect gate="G$1" pin="DR1SEC" pad="F3"/>
<connect gate="G$1" pin="DT0PRI" pad="H1"/>
<connect gate="G$1" pin="DT0SEC" pad="H2"/>
<connect gate="G$1" pin="DT1PRI" pad="F2"/>
<connect gate="G$1" pin="DT1SEC" pad="E3"/>
<connect gate="G$1" pin="EMU_B" pad="M2"/>
<connect gate="G$1" pin="GND@0" pad="H4"/>
<connect gate="G$1" pin="GND@1" pad="A14"/>
<connect gate="G$1" pin="GND@10" pad="L5"/>
<connect gate="G$1" pin="GND@11" pad="P14"/>
<connect gate="G$1" pin="GND@12" pad="C4"/>
<connect gate="G$1" pin="GND@13" pad="D10"/>
<connect gate="G$1" pin="GND@14" pad="L6"/>
<connect gate="G$1" pin="GND@15" pad="C5"/>
<connect gate="G$1" pin="GND@16" pad="D7"/>
<connect gate="G$1" pin="GND@17" pad="F11"/>
<connect gate="G$1" pin="GND@18" pad="D4"/>
<connect gate="G$1" pin="GND@19" pad="K4"/>
<connect gate="G$1" pin="GND@2" pad="D11"/>
<connect gate="G$1" pin="GND@20" pad="K11"/>
<connect gate="G$1" pin="GND@21" pad="L8"/>
<connect gate="G$1" pin="GND@22" pad="A10"/>
<connect gate="G$1" pin="GND@23" pad="B11"/>
<connect gate="G$1" pin="GND@3" pad="L10"/>
<connect gate="G$1" pin="GND@4" pad="C11"/>
<connect gate="G$1" pin="GND@5" pad="H11"/>
<connect gate="G$1" pin="GND@6" pad="F4"/>
<connect gate="G$1" pin="GND@7" pad="G11"/>
<connect gate="G$1" pin="GND@8" pad="M10"/>
<connect gate="G$1" pin="GND@9" pad="D8"/>
<connect gate="G$1" pin="MISO" pad="E2"/>
<connect gate="G$1" pin="MOSI" pad="D3"/>
<connect gate="G$1" pin="NMI" pad="B10"/>
<connect gate="G$1" pin="PF0" pad="D2"/>
<connect gate="G$1" pin="PF1" pad="C1"/>
<connect gate="G$1" pin="PF10" pad="A4"/>
<connect gate="G$1" pin="PF11" pad="A5"/>
<connect gate="G$1" pin="PF12" pad="B5"/>
<connect gate="G$1" pin="PF13" pad="B6"/>
<connect gate="G$1" pin="PF14" pad="A6"/>
<connect gate="G$1" pin="PF15" pad="C6"/>
<connect gate="G$1" pin="PF2" pad="C2"/>
<connect gate="G$1" pin="PF3" pad="C3"/>
<connect gate="G$1" pin="PF4" pad="B1"/>
<connect gate="G$1" pin="PF5" pad="B2"/>
<connect gate="G$1" pin="PF6" pad="B3"/>
<connect gate="G$1" pin="PF7" pad="B4"/>
<connect gate="G$1" pin="PF8" pad="A2"/>
<connect gate="G$1" pin="PF9" pad="A3"/>
<connect gate="G$1" pin="PP0" pad="C8"/>
<connect gate="G$1" pin="PP1" pad="B8"/>
<connect gate="G$1" pin="PP2" pad="A7"/>
<connect gate="G$1" pin="PP3" pad="B7"/>
<connect gate="G$1" pin="PP_CLK" pad="C9"/>
<connect gate="G$1" pin="RESET_B" pad="C10"/>
<connect gate="G$1" pin="RFS0" pad="J3"/>
<connect gate="G$1" pin="RFS1" pad="G2"/>
<connect gate="G$1" pin="RSCLK0" pad="L1"/>
<connect gate="G$1" pin="RSCLK1" pad="G1"/>
<connect gate="G$1" pin="RTXI" pad="A9"/>
<connect gate="G$1" pin="RTXO" pad="A8"/>
<connect gate="G$1" pin="RX" pad="L3"/>
<connect gate="G$1" pin="SA10" pad="E12"/>
<connect gate="G$1" pin="SCAS_B" pad="C14"/>
<connect gate="G$1" pin="SCK" pad="D1"/>
<connect gate="G$1" pin="SCKE" pad="B13"/>
<connect gate="G$1" pin="SMS_B" pad="C13"/>
<connect gate="G$1" pin="SRAS_B" pad="D13"/>
<connect gate="G$1" pin="SWE_B" pad="D12"/>
<connect gate="G$1" pin="TCK" pad="P2"/>
<connect gate="G$1" pin="TDI" pad="M3"/>
<connect gate="G$1" pin="TDO" pad="N3"/>
<connect gate="G$1" pin="TEST" pad="M4"/>
<connect gate="G$1" pin="TFS0" pad="H3"/>
<connect gate="G$1" pin="TFS1" pad="E1"/>
<connect gate="G$1" pin="TMR0" pad="L2"/>
<connect gate="G$1" pin="TMR1" pad="M1"/>
<connect gate="G$1" pin="TMR2" pad="K2"/>
<connect gate="G$1" pin="TMS" pad="N2"/>
<connect gate="G$1" pin="TRST_B" pad="N1"/>
<connect gate="G$1" pin="TSCLK0" pad="J1"/>
<connect gate="G$1" pin="TSCLK1" pad="F1"/>
<connect gate="G$1" pin="TX" pad="K3"/>
<connect gate="G$1" pin="VDD_EXT@0" pad="J12"/>
<connect gate="G$1" pin="VDD_EXT@1" pad="F12"/>
<connect gate="G$1" pin="VDD_EXT@10" pad="G4"/>
<connect gate="G$1" pin="VDD_EXT@11" pad="C12"/>
<connect gate="G$1" pin="VDD_EXT@2" pad="C7"/>
<connect gate="G$1" pin="VDD_EXT@3" pad="A1"/>
<connect gate="G$1" pin="VDD_EXT@4" pad="P1"/>
<connect gate="G$1" pin="VDD_EXT@5" pad="J4"/>
<connect gate="G$1" pin="VDD_EXT@6" pad="D9"/>
<connect gate="G$1" pin="VDD_EXT@7" pad="L11"/>
<connect gate="G$1" pin="VDD_EXT@8" pad="L7"/>
<connect gate="G$1" pin="VDD_EXT@9" pad="D5"/>
<connect gate="G$1" pin="VDD_INT@0" pad="J11"/>
<connect gate="G$1" pin="VDD_INT@1" pad="D6"/>
<connect gate="G$1" pin="VDD_INT@2" pad="E4"/>
<connect gate="G$1" pin="VDD_INT@3" pad="E11"/>
<connect gate="G$1" pin="VDD_INT@4" pad="L9"/>
<connect gate="G$1" pin="VDD_INT@5" pad="L4"/>
<connect gate="G$1" pin="VDD_RTC" pad="B9"/>
<connect gate="G$1" pin="VROUT@0" pad="A13"/>
<connect gate="G$1" pin="VROUT@1" pad="B12"/>
<connect gate="G$1" pin="XTAL" pad="A11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_BF532" prefix="IC">
<description>&lt;b&gt;ADSP BF532&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 8&lt;/i&gt;&lt;br&gt;
Source: 33335272594765ADSP_BF532_mbga.bsdl</description>
<gates>
<gate name="G$1" symbol="33335272594765ADSP_BF532_MBGA"/>
</gates>
<devices>
<device name="" package="MBGA_160">
<connects>
<connect gate="G$1" pin="ABE_B0" pad="H13"/>
<connect gate="G$1" pin="ABE_B1" pad="H12"/>
<connect gate="G$1" pin="ADDR1" pad="J14"/>
<connect gate="G$1" pin="ADDR10" pad="M13"/>
<connect gate="G$1" pin="ADDR11" pad="M14"/>
<connect gate="G$1" pin="ADDR12" pad="N14"/>
<connect gate="G$1" pin="ADDR13" pad="N13"/>
<connect gate="G$1" pin="ADDR14" pad="N12"/>
<connect gate="G$1" pin="ADDR15" pad="M11"/>
<connect gate="G$1" pin="ADDR16" pad="N11"/>
<connect gate="G$1" pin="ADDR17" pad="P13"/>
<connect gate="G$1" pin="ADDR18" pad="P12"/>
<connect gate="G$1" pin="ADDR19" pad="P11"/>
<connect gate="G$1" pin="ADDR2" pad="K14"/>
<connect gate="G$1" pin="ADDR3" pad="L14"/>
<connect gate="G$1" pin="ADDR4" pad="J13"/>
<connect gate="G$1" pin="ADDR5" pad="K13"/>
<connect gate="G$1" pin="ADDR6" pad="L13"/>
<connect gate="G$1" pin="ADDR7" pad="K12"/>
<connect gate="G$1" pin="ADDR8" pad="L12"/>
<connect gate="G$1" pin="ADDR9" pad="M12"/>
<connect gate="G$1" pin="AMS_B0" pad="E14"/>
<connect gate="G$1" pin="AMS_B1" pad="F14"/>
<connect gate="G$1" pin="AMS_B2" pad="F13"/>
<connect gate="G$1" pin="AMS_B3" pad="G12"/>
<connect gate="G$1" pin="AOE_B" pad="G13"/>
<connect gate="G$1" pin="ARDY" pad="E13"/>
<connect gate="G$1" pin="ARE_B" pad="G14"/>
<connect gate="G$1" pin="AWE_B" pad="H14"/>
<connect gate="G$1" pin="BGH_B" pad="N10"/>
<connect gate="G$1" pin="BG_B" pad="P10"/>
<connect gate="G$1" pin="BMODE0" pad="N4"/>
<connect gate="G$1" pin="BMODE1" pad="P3"/>
<connect gate="G$1" pin="BR_B" pad="D14"/>
<connect gate="G$1" pin="CLKIN" pad="A12"/>
<connect gate="G$1" pin="CLKOUT" pad="B14"/>
<connect gate="G$1" pin="DATA0" pad="M9"/>
<connect gate="G$1" pin="DATA1" pad="N9"/>
<connect gate="G$1" pin="DATA10" pad="N6"/>
<connect gate="G$1" pin="DATA11" pad="P6"/>
<connect gate="G$1" pin="DATA12" pad="M5"/>
<connect gate="G$1" pin="DATA13" pad="N5"/>
<connect gate="G$1" pin="DATA14" pad="P5"/>
<connect gate="G$1" pin="DATA15" pad="P4"/>
<connect gate="G$1" pin="DATA2" pad="P9"/>
<connect gate="G$1" pin="DATA3" pad="M8"/>
<connect gate="G$1" pin="DATA4" pad="N8"/>
<connect gate="G$1" pin="DATA5" pad="P8"/>
<connect gate="G$1" pin="DATA6" pad="M7"/>
<connect gate="G$1" pin="DATA7" pad="N7"/>
<connect gate="G$1" pin="DATA8" pad="P7"/>
<connect gate="G$1" pin="DATA9" pad="M6"/>
<connect gate="G$1" pin="DR0PRI" pad="K1"/>
<connect gate="G$1" pin="DR0SEC" pad="J2"/>
<connect gate="G$1" pin="DR1PRI" pad="G3"/>
<connect gate="G$1" pin="DR1SEC" pad="F3"/>
<connect gate="G$1" pin="DT0PRI" pad="H1"/>
<connect gate="G$1" pin="DT0SEC" pad="H2"/>
<connect gate="G$1" pin="DT1PRI" pad="F2"/>
<connect gate="G$1" pin="DT1SEC" pad="E3"/>
<connect gate="G$1" pin="EMU_B" pad="M2"/>
<connect gate="G$1" pin="GND@0" pad="H4"/>
<connect gate="G$1" pin="GND@1" pad="A14"/>
<connect gate="G$1" pin="GND@10" pad="L5"/>
<connect gate="G$1" pin="GND@11" pad="P14"/>
<connect gate="G$1" pin="GND@12" pad="C4"/>
<connect gate="G$1" pin="GND@13" pad="D10"/>
<connect gate="G$1" pin="GND@14" pad="L6"/>
<connect gate="G$1" pin="GND@15" pad="C5"/>
<connect gate="G$1" pin="GND@16" pad="D7"/>
<connect gate="G$1" pin="GND@17" pad="F11"/>
<connect gate="G$1" pin="GND@18" pad="D4"/>
<connect gate="G$1" pin="GND@19" pad="K4"/>
<connect gate="G$1" pin="GND@2" pad="D11"/>
<connect gate="G$1" pin="GND@20" pad="K11"/>
<connect gate="G$1" pin="GND@21" pad="L8"/>
<connect gate="G$1" pin="GND@22" pad="A10"/>
<connect gate="G$1" pin="GND@23" pad="B11"/>
<connect gate="G$1" pin="GND@3" pad="L10"/>
<connect gate="G$1" pin="GND@4" pad="C11"/>
<connect gate="G$1" pin="GND@5" pad="H11"/>
<connect gate="G$1" pin="GND@6" pad="F4"/>
<connect gate="G$1" pin="GND@7" pad="G11"/>
<connect gate="G$1" pin="GND@8" pad="M10"/>
<connect gate="G$1" pin="GND@9" pad="D8"/>
<connect gate="G$1" pin="MISO" pad="E2"/>
<connect gate="G$1" pin="MOSI" pad="D3"/>
<connect gate="G$1" pin="NMI" pad="B10"/>
<connect gate="G$1" pin="PF0" pad="D2"/>
<connect gate="G$1" pin="PF1" pad="C1"/>
<connect gate="G$1" pin="PF10" pad="A4"/>
<connect gate="G$1" pin="PF11" pad="A5"/>
<connect gate="G$1" pin="PF12" pad="B5"/>
<connect gate="G$1" pin="PF13" pad="B6"/>
<connect gate="G$1" pin="PF14" pad="A6"/>
<connect gate="G$1" pin="PF15" pad="C6"/>
<connect gate="G$1" pin="PF2" pad="C2"/>
<connect gate="G$1" pin="PF3" pad="C3"/>
<connect gate="G$1" pin="PF4" pad="B1"/>
<connect gate="G$1" pin="PF5" pad="B2"/>
<connect gate="G$1" pin="PF6" pad="B3"/>
<connect gate="G$1" pin="PF7" pad="B4"/>
<connect gate="G$1" pin="PF8" pad="A2"/>
<connect gate="G$1" pin="PF9" pad="A3"/>
<connect gate="G$1" pin="PP0" pad="C8"/>
<connect gate="G$1" pin="PP1" pad="B8"/>
<connect gate="G$1" pin="PP2" pad="A7"/>
<connect gate="G$1" pin="PP3" pad="B7"/>
<connect gate="G$1" pin="PP_CLK" pad="C9"/>
<connect gate="G$1" pin="RESET_B" pad="C10"/>
<connect gate="G$1" pin="RFS0" pad="J3"/>
<connect gate="G$1" pin="RFS1" pad="G2"/>
<connect gate="G$1" pin="RSCLK0" pad="L1"/>
<connect gate="G$1" pin="RSCLK1" pad="G1"/>
<connect gate="G$1" pin="RTXI" pad="A9"/>
<connect gate="G$1" pin="RTXO" pad="A8"/>
<connect gate="G$1" pin="RX" pad="L3"/>
<connect gate="G$1" pin="SA10" pad="E12"/>
<connect gate="G$1" pin="SCAS_B" pad="C14"/>
<connect gate="G$1" pin="SCK" pad="D1"/>
<connect gate="G$1" pin="SCKE" pad="B13"/>
<connect gate="G$1" pin="SMS_B" pad="C13"/>
<connect gate="G$1" pin="SRAS_B" pad="D13"/>
<connect gate="G$1" pin="SWE_B" pad="D12"/>
<connect gate="G$1" pin="TCK" pad="P2"/>
<connect gate="G$1" pin="TDI" pad="M3"/>
<connect gate="G$1" pin="TDO" pad="N3"/>
<connect gate="G$1" pin="TEST" pad="M4"/>
<connect gate="G$1" pin="TFS0" pad="H3"/>
<connect gate="G$1" pin="TFS1" pad="E1"/>
<connect gate="G$1" pin="TMR0" pad="L2"/>
<connect gate="G$1" pin="TMR1" pad="M1"/>
<connect gate="G$1" pin="TMR2" pad="K2"/>
<connect gate="G$1" pin="TMS" pad="N2"/>
<connect gate="G$1" pin="TRST_B" pad="N1"/>
<connect gate="G$1" pin="TSCLK0" pad="J1"/>
<connect gate="G$1" pin="TSCLK1" pad="F1"/>
<connect gate="G$1" pin="TX" pad="K3"/>
<connect gate="G$1" pin="VDD_EXT@0" pad="J12"/>
<connect gate="G$1" pin="VDD_EXT@1" pad="F12"/>
<connect gate="G$1" pin="VDD_EXT@10" pad="G4"/>
<connect gate="G$1" pin="VDD_EXT@11" pad="C12"/>
<connect gate="G$1" pin="VDD_EXT@2" pad="C7"/>
<connect gate="G$1" pin="VDD_EXT@3" pad="A1"/>
<connect gate="G$1" pin="VDD_EXT@4" pad="P1"/>
<connect gate="G$1" pin="VDD_EXT@5" pad="J4"/>
<connect gate="G$1" pin="VDD_EXT@6" pad="D9"/>
<connect gate="G$1" pin="VDD_EXT@7" pad="L11"/>
<connect gate="G$1" pin="VDD_EXT@8" pad="L7"/>
<connect gate="G$1" pin="VDD_EXT@9" pad="D5"/>
<connect gate="G$1" pin="VDD_INT@0" pad="J11"/>
<connect gate="G$1" pin="VDD_INT@1" pad="D6"/>
<connect gate="G$1" pin="VDD_INT@2" pad="E4"/>
<connect gate="G$1" pin="VDD_INT@3" pad="E11"/>
<connect gate="G$1" pin="VDD_INT@4" pad="L9"/>
<connect gate="G$1" pin="VDD_INT@5" pad="L4"/>
<connect gate="G$1" pin="VDD_RTC" pad="B9"/>
<connect gate="G$1" pin="VROUT@0" pad="A13"/>
<connect gate="G$1" pin="VROUT@1" pad="B12"/>
<connect gate="G$1" pin="XTAL" pad="A11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_BF537" prefix="IC">
<description>&lt;b&gt;ADSP-BF534-BSDL_br.txt.bsdl&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 8&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/90140778ADSP_BF536_7_prd.pdf&lt;br&gt;
Source2: BSDL_br.txt as Email: &amp;lt;adi-germany@analog.com&amp;gt;</description>
<gates>
<gate name="G$1" symbol="ADSP-BF537"/>
</gates>
<devices>
<device name="" package="BGA_208">
<connects>
<connect gate="G$1" pin="ABE_B0" pad="P19"/>
<connect gate="G$1" pin="ABE_B1" pad="P20"/>
<connect gate="G$1" pin="ADDR1" pad="R19"/>
<connect gate="G$1" pin="ADDR10" pad="W18"/>
<connect gate="G$1" pin="ADDR11" pad="X18"/>
<connect gate="G$1" pin="ADDR12" pad="W17"/>
<connect gate="G$1" pin="ADDR13" pad="X17"/>
<connect gate="G$1" pin="ADDR14" pad="W16"/>
<connect gate="G$1" pin="ADDR15" pad="X16"/>
<connect gate="G$1" pin="ADDR16" pad="W15"/>
<connect gate="G$1" pin="ADDR17" pad="X15"/>
<connect gate="G$1" pin="ADDR18" pad="W14"/>
<connect gate="G$1" pin="ADDR19" pad="X14"/>
<connect gate="G$1" pin="ADDR2" pad="T20"/>
<connect gate="G$1" pin="ADDR3" pad="T19"/>
<connect gate="G$1" pin="ADDR4" pad="U20"/>
<connect gate="G$1" pin="ADDR5" pad="U19"/>
<connect gate="G$1" pin="ADDR6" pad="V20"/>
<connect gate="G$1" pin="ADDR7" pad="V19"/>
<connect gate="G$1" pin="ADDR8" pad="W20"/>
<connect gate="G$1" pin="ADDR9" pad="X19"/>
<connect gate="G$1" pin="AMS_B0" pad="M20"/>
<connect gate="G$1" pin="AMS_B1" pad="M19"/>
<connect gate="G$1" pin="AMS_B2" pad="G20"/>
<connect gate="G$1" pin="AMS_B3" pad="G19"/>
<connect gate="G$1" pin="AOE_B" pad="N20"/>
<connect gate="G$1" pin="ARDY" pad="J19"/>
<connect gate="G$1" pin="ARE_B" pad="N19"/>
<connect gate="G$1" pin="AWE_B" pad="R20"/>
<connect gate="G$1" pin="BGH_B" pad="X12"/>
<connect gate="G$1" pin="BG_B" pad="X11"/>
<connect gate="G$1" pin="BMODE0" pad="W13"/>
<connect gate="G$1" pin="BMODE1" pad="W12"/>
<connect gate="G$1" pin="BMODE2" pad="W11"/>
<connect gate="G$1" pin="BR_B" pad="F19"/>
<connect gate="G$1" pin="BUF_XTAL" pad="B14"/>
<connect gate="G$1" pin="CLKIN" pad="A18"/>
<connect gate="G$1" pin="CLKOUT" pad="H19"/>
<connect gate="G$1" pin="DATA0" pad="X10"/>
<connect gate="G$1" pin="DATA1" pad="W10"/>
<connect gate="G$1" pin="DATA10" pad="X5"/>
<connect gate="G$1" pin="DATA11" pad="W5"/>
<connect gate="G$1" pin="DATA12" pad="X4"/>
<connect gate="G$1" pin="DATA13" pad="W4"/>
<connect gate="G$1" pin="DATA14" pad="X3"/>
<connect gate="G$1" pin="DATA15" pad="W3"/>
<connect gate="G$1" pin="DATA2" pad="X9"/>
<connect gate="G$1" pin="DATA3" pad="W9"/>
<connect gate="G$1" pin="DATA4" pad="X8"/>
<connect gate="G$1" pin="DATA5" pad="W8"/>
<connect gate="G$1" pin="DATA6" pad="X7"/>
<connect gate="G$1" pin="DATA7" pad="W7"/>
<connect gate="G$1" pin="DATA8" pad="X6"/>
<connect gate="G$1" pin="DATA9" pad="W6"/>
<connect gate="G$1" pin="DR0PRI" pad="B17"/>
<connect gate="G$1" pin="DR0SEC" pad="B18"/>
<connect gate="G$1" pin="DT0PRI" pad="C19"/>
<connect gate="G$1" pin="DT0SEC" pad="A19"/>
<connect gate="G$1" pin="EMU_B" pad="T1"/>
<connect gate="G$1" pin="GND@0" pad="A1"/>
<connect gate="G$1" pin="GND@1" pad="A13"/>
<connect gate="G$1" pin="GND@10" pad="J10"/>
<connect gate="G$1" pin="GND@11" pad="J11"/>
<connect gate="G$1" pin="GND@12" pad="J12"/>
<connect gate="G$1" pin="GND@13" pad="J13"/>
<connect gate="G$1" pin="GND@14" pad="K9"/>
<connect gate="G$1" pin="GND@15" pad="K10"/>
<connect gate="G$1" pin="GND@16" pad="K11"/>
<connect gate="G$1" pin="GND@17" pad="K12"/>
<connect gate="G$1" pin="GND@18" pad="K13"/>
<connect gate="G$1" pin="GND@19" pad="L9"/>
<connect gate="G$1" pin="GND@2" pad="A20"/>
<connect gate="G$1" pin="GND@20" pad="L10"/>
<connect gate="G$1" pin="GND@21" pad="L11"/>
<connect gate="G$1" pin="GND@22" pad="L12"/>
<connect gate="G$1" pin="GND@23" pad="L13"/>
<connect gate="G$1" pin="GND@24" pad="M9"/>
<connect gate="G$1" pin="GND@25" pad="M10"/>
<connect gate="G$1" pin="GND@26" pad="M11"/>
<connect gate="G$1" pin="GND@27" pad="M12"/>
<connect gate="G$1" pin="GND@28" pad="M13"/>
<connect gate="G$1" pin="GND@29" pad="N9"/>
<connect gate="G$1" pin="GND@3" pad="G11"/>
<connect gate="G$1" pin="GND@30" pad="N10"/>
<connect gate="G$1" pin="GND@31" pad="N11"/>
<connect gate="G$1" pin="GND@32" pad="N12"/>
<connect gate="G$1" pin="GND@33" pad="N13"/>
<connect gate="G$1" pin="GND@34" pad="P11"/>
<connect gate="G$1" pin="GND@35" pad="X1"/>
<connect gate="G$1" pin="GND@36" pad="X20"/>
<connect gate="G$1" pin="GND@4" pad="H9"/>
<connect gate="G$1" pin="GND@5" pad="H10"/>
<connect gate="G$1" pin="GND@6" pad="H11"/>
<connect gate="G$1" pin="GND@7" pad="H12"/>
<connect gate="G$1" pin="GND@8" pad="H13"/>
<connect gate="G$1" pin="GND@9" pad="J9"/>
<connect gate="G$1" pin="MDC" pad="B12"/>
<connect gate="G$1" pin="MDIO" pad="B13"/>
<connect gate="G$1" pin="NMI" pad="C20"/>
<connect gate="G$1" pin="PF0" pad="H2"/>
<connect gate="G$1" pin="PF1" pad="G1"/>
<connect gate="G$1" pin="PF10" pad="C2"/>
<connect gate="G$1" pin="PF11" pad="B1"/>
<connect gate="G$1" pin="PF12" pad="A2"/>
<connect gate="G$1" pin="PF13" pad="A3"/>
<connect gate="G$1" pin="PF14" pad="B3"/>
<connect gate="G$1" pin="PF15" pad="A4"/>
<connect gate="G$1" pin="PF16" pad="T2"/>
<connect gate="G$1" pin="PF17" pad="R1"/>
<connect gate="G$1" pin="PF18" pad="R2"/>
<connect gate="G$1" pin="PF19" pad="P1"/>
<connect gate="G$1" pin="PF2" pad="G2"/>
<connect gate="G$1" pin="PF20" pad="P2"/>
<connect gate="G$1" pin="PF21" pad="N1"/>
<connect gate="G$1" pin="PF22" pad="N2"/>
<connect gate="G$1" pin="PF23" pad="M1"/>
<connect gate="G$1" pin="PF24" pad="M2"/>
<connect gate="G$1" pin="PF25" pad="L1"/>
<connect gate="G$1" pin="PF26" pad="L2"/>
<connect gate="G$1" pin="PF27" pad="K1"/>
<connect gate="G$1" pin="PF28" pad="K2"/>
<connect gate="G$1" pin="PF29" pad="J1"/>
<connect gate="G$1" pin="PF3" pad="F1"/>
<connect gate="G$1" pin="PF30" pad="J2"/>
<connect gate="G$1" pin="PF31" pad="H1"/>
<connect gate="G$1" pin="PF32" pad="B4"/>
<connect gate="G$1" pin="PF33" pad="A5"/>
<connect gate="G$1" pin="PF34" pad="A6"/>
<connect gate="G$1" pin="PF35" pad="B5"/>
<connect gate="G$1" pin="PF36" pad="B6"/>
<connect gate="G$1" pin="PF37" pad="A7"/>
<connect gate="G$1" pin="PF38" pad="B7"/>
<connect gate="G$1" pin="PF39" pad="A8"/>
<connect gate="G$1" pin="PF4" pad="F2"/>
<connect gate="G$1" pin="PF40" pad="B8"/>
<connect gate="G$1" pin="PF41" pad="A9"/>
<connect gate="G$1" pin="PF42" pad="B9"/>
<connect gate="G$1" pin="PF43" pad="A10"/>
<connect gate="G$1" pin="PF44" pad="B10"/>
<connect gate="G$1" pin="PF45" pad="A11"/>
<connect gate="G$1" pin="PF46" pad="B11"/>
<connect gate="G$1" pin="PF47" pad="A12"/>
<connect gate="G$1" pin="PF5" pad="E1"/>
<connect gate="G$1" pin="PF6" pad="E2"/>
<connect gate="G$1" pin="PF7" pad="D1"/>
<connect gate="G$1" pin="PF8" pad="D2"/>
<connect gate="G$1" pin="PF9" pad="C1"/>
<connect gate="G$1" pin="RESET_B" pad="D20"/>
<connect gate="G$1" pin="RFS0" pad="B16"/>
<connect gate="G$1" pin="RSCLK0" pad="B15"/>
<connect gate="G$1" pin="RTXI" pad="A14"/>
<connect gate="G$1" pin="RTXO" pad="A15"/>
<connect gate="G$1" pin="SA10" pad="L20"/>
<connect gate="G$1" pin="SCAS_B" pad="K20"/>
<connect gate="G$1" pin="SCKE" pad="H20"/>
<connect gate="G$1" pin="SCL" pad="D19"/>
<connect gate="G$1" pin="SDA" pad="E19"/>
<connect gate="G$1" pin="SMS_B" pad="J20"/>
<connect gate="G$1" pin="SRAS_B" pad="K19"/>
<connect gate="G$1" pin="SWE_B" pad="L19"/>
<connect gate="G$1" pin="TCK" pad="W1"/>
<connect gate="G$1" pin="TDI" pad="V1"/>
<connect gate="G$1" pin="TDO" pad="X2"/>
<connect gate="G$1" pin="TEST" pad="V2"/>
<connect gate="G$1" pin="TFS0" pad="B19"/>
<connect gate="G$1" pin="TMS" pad="U2"/>
<connect gate="G$1" pin="TRST_B" pad="U1"/>
<connect gate="G$1" pin="TSCLK0" pad="B20"/>
<connect gate="G$1" pin="VDD_EXT@0" pad="G7"/>
<connect gate="G$1" pin="VDD_EXT@1" pad="G8"/>
<connect gate="G$1" pin="VDD_EXT@10" pad="L7"/>
<connect gate="G$1" pin="VDD_EXT@11" pad="L8"/>
<connect gate="G$1" pin="VDD_EXT@12" pad="M7"/>
<connect gate="G$1" pin="VDD_EXT@13" pad="M8"/>
<connect gate="G$1" pin="VDD_EXT@14" pad="N7"/>
<connect gate="G$1" pin="VDD_EXT@15" pad="N8"/>
<connect gate="G$1" pin="VDD_EXT@16" pad="P7"/>
<connect gate="G$1" pin="VDD_EXT@17" pad="P8"/>
<connect gate="G$1" pin="VDD_EXT@18" pad="P9"/>
<connect gate="G$1" pin="VDD_EXT@19" pad="P10"/>
<connect gate="G$1" pin="VDD_EXT@2" pad="G9"/>
<connect gate="G$1" pin="VDD_EXT@3" pad="G10"/>
<connect gate="G$1" pin="VDD_EXT@4" pad="H7"/>
<connect gate="G$1" pin="VDD_EXT@5" pad="H8"/>
<connect gate="G$1" pin="VDD_EXT@6" pad="J7"/>
<connect gate="G$1" pin="VDD_EXT@7" pad="J8"/>
<connect gate="G$1" pin="VDD_EXT@8" pad="K7"/>
<connect gate="G$1" pin="VDD_EXT@9" pad="K8"/>
<connect gate="G$1" pin="VDD_INT@0" pad="G12"/>
<connect gate="G$1" pin="VDD_INT@1" pad="G13"/>
<connect gate="G$1" pin="VDD_INT@10" pad="P13"/>
<connect gate="G$1" pin="VDD_INT@11" pad="P14"/>
<connect gate="G$1" pin="VDD_INT@2" pad="G14"/>
<connect gate="G$1" pin="VDD_INT@3" pad="H14"/>
<connect gate="G$1" pin="VDD_INT@4" pad="J14"/>
<connect gate="G$1" pin="VDD_INT@5" pad="K14"/>
<connect gate="G$1" pin="VDD_INT@6" pad="L14"/>
<connect gate="G$1" pin="VDD_INT@7" pad="M14"/>
<connect gate="G$1" pin="VDD_INT@8" pad="N14"/>
<connect gate="G$1" pin="VDD_INT@9" pad="P12"/>
<connect gate="G$1" pin="VDD_RTC" pad="A16"/>
<connect gate="G$1" pin="VROUT@0" pad="E20"/>
<connect gate="G$1" pin="VROUT@1" pad="F20"/>
<connect gate="G$1" pin="XTAL" pad="A17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADSP-BF537BBCZ-5B"/>
<attribute name="OC_FARNELL" value="1776215"/>
<attribute name="OC_NEWARK" value="31M8122"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADD8704" prefix="IC">
<description>&lt;b&gt;16 V Quad Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: Ananlog Devices .. 780914713ADD8704_0.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="C" symbol="OP"/>
<gate name="D" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="CP" package="LFCSP16">
<connects>
<connect gate="A" pin="IN+" pad="2"/>
<connect gate="A" pin="IN-" pad="1"/>
<connect gate="A" pin="OUT" pad="15"/>
<connect gate="B" pin="IN+" pad="4"/>
<connect gate="B" pin="IN-" pad="5"/>
<connect gate="B" pin="OUT" pad="6"/>
<connect gate="C" pin="IN+" pad="9"/>
<connect gate="C" pin="IN-" pad="8"/>
<connect gate="C" pin="OUT" pad="7"/>
<connect gate="D" pin="IN+" pad="11"/>
<connect gate="D" pin="IN-" pad="12"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADD8704ACPZ-REEL7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K0961"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP14">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="IN+" pad="10"/>
<connect gate="C" pin="IN-" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="IN+" pad="12"/>
<connect gate="D" pin="IN-" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADD8704ARUZ-REEL"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K0964"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_BF535" prefix="IC">
<description>&lt;b&gt;Blackfin® Embedded Processor ADSP 535&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 11&lt;/i&gt;&lt;br&gt;
Source: ADSP_21535.bsdl&lt;br&gt;
http://www.analog.com/UploadedFiles/Data_Sheets/744511807ADSP_BF535_a.pdf</description>
<gates>
<gate name="G$1" symbol="ADSP_21535"/>
</gates>
<devices>
<device name="" package="PBGA_B260">
<connects>
<connect gate="G$1" pin="ABE_B_SDQM0" pad="E2"/>
<connect gate="G$1" pin="ABE_B_SDQM1" pad="B1"/>
<connect gate="G$1" pin="ABE_B_SDQM2" pad="G3"/>
<connect gate="G$1" pin="ABE_B_SDQM3" pad="H7"/>
<connect gate="G$1" pin="ADDR10" pad="D5"/>
<connect gate="G$1" pin="ADDR11" pad="B4"/>
<connect gate="G$1" pin="ADDR12" pad="A1"/>
<connect gate="G$1" pin="ADDR13" pad="C4"/>
<connect gate="G$1" pin="ADDR14" pad="D4"/>
<connect gate="G$1" pin="ADDR15" pad="A3"/>
<connect gate="G$1" pin="ADDR16" pad="B3"/>
<connect gate="G$1" pin="ADDR17" pad="A2"/>
<connect gate="G$1" pin="ADDR18" pad="C3"/>
<connect gate="G$1" pin="ADDR19" pad="D3"/>
<connect gate="G$1" pin="ADDR2" pad="A6"/>
<connect gate="G$1" pin="ADDR20" pad="B2"/>
<connect gate="G$1" pin="ADDR21" pad="C2"/>
<connect gate="G$1" pin="ADDR22" pad="E3"/>
<connect gate="G$1" pin="ADDR23" pad="C1"/>
<connect gate="G$1" pin="ADDR24" pad="F3"/>
<connect gate="G$1" pin="ADDR25" pad="D2"/>
<connect gate="G$1" pin="ADDR3" pad="B6"/>
<connect gate="G$1" pin="ADDR4" pad="D6"/>
<connect gate="G$1" pin="ADDR5" pad="C6"/>
<connect gate="G$1" pin="ADDR6" pad="A5"/>
<connect gate="G$1" pin="ADDR7" pad="B5"/>
<connect gate="G$1" pin="ADDR8" pad="A4"/>
<connect gate="G$1" pin="ADDR9" pad="C5"/>
<connect gate="G$1" pin="AMS_B0" pad="F2"/>
<connect gate="G$1" pin="AMS_B1" pad="D1"/>
<connect gate="G$1" pin="AMS_B2" pad="H3"/>
<connect gate="G$1" pin="AMS_B3" pad="G2"/>
<connect gate="G$1" pin="AOE_B" pad="E1"/>
<connect gate="G$1" pin="ARDY" pad="R1"/>
<connect gate="G$1" pin="ARE_B" pad="F1"/>
<connect gate="G$1" pin="AWE_B" pad="G1"/>
<connect gate="G$1" pin="BMODE0" pad="B14"/>
<connect gate="G$1" pin="BMODE1" pad="A14"/>
<connect gate="G$1" pin="BMODE2" pad="B13"/>
<connect gate="G$1" pin="BYPASS" pad="C12"/>
<connect gate="G$1" pin="CLKIN1" pad="D9"/>
<connect gate="G$1" pin="CLKOUT_SCLK1" pad="H1"/>
<connect gate="G$1" pin="DATA0" pad="N2"/>
<connect gate="G$1" pin="DATA1" pad="M3"/>
<connect gate="G$1" pin="DATA10" pad="V2"/>
<connect gate="G$1" pin="DATA11" pad="V3"/>
<connect gate="G$1" pin="DATA12" pad="R4"/>
<connect gate="G$1" pin="DATA13" pad="U3"/>
<connect gate="G$1" pin="DATA14" pad="T3"/>
<connect gate="G$1" pin="DATA15" pad="T4"/>
<connect gate="G$1" pin="DATA16" pad="U4"/>
<connect gate="G$1" pin="DATA17" pad="V4"/>
<connect gate="G$1" pin="DATA18" pad="V5"/>
<connect gate="G$1" pin="DATA19" pad="R5"/>
<connect gate="G$1" pin="DATA2" pad="T1"/>
<connect gate="G$1" pin="DATA20" pad="T5"/>
<connect gate="G$1" pin="DATA21" pad="U5"/>
<connect gate="G$1" pin="DATA22" pad="V6"/>
<connect gate="G$1" pin="DATA23" pad="R6"/>
<connect gate="G$1" pin="DATA24" pad="U6"/>
<connect gate="G$1" pin="DATA25" pad="T6"/>
<connect gate="G$1" pin="DATA26" pad="V7"/>
<connect gate="G$1" pin="DATA27" pad="V8"/>
<connect gate="G$1" pin="DATA28" pad="U7"/>
<connect gate="G$1" pin="DATA29" pad="R7"/>
<connect gate="G$1" pin="DATA3" pad="P2"/>
<connect gate="G$1" pin="DATA30" pad="T7"/>
<connect gate="G$1" pin="DATA31" pad="V9"/>
<connect gate="G$1" pin="DATA4" pad="N3"/>
<connect gate="G$1" pin="DATA5" pad="R2"/>
<connect gate="G$1" pin="DATA6" pad="P3"/>
<connect gate="G$1" pin="DATA7" pad="U1"/>
<connect gate="G$1" pin="DATA8" pad="U2"/>
<connect gate="G$1" pin="DATA9" pad="T2"/>
<connect gate="G$1" pin="DMNS" pad="D8"/>
<connect gate="G$1" pin="DPLS" pad="C9"/>
<connect gate="G$1" pin="DR0" pad="V14"/>
<connect gate="G$1" pin="DR1" pad="U15"/>
<connect gate="G$1" pin="DT0" pad="R14"/>
<connect gate="G$1" pin="DT1" pad="V17"/>
<connect gate="G$1" pin="EMU_B" pad="A13"/>
<connect gate="G$1" pin="GND@0" pad="C13"/>
<connect gate="G$1" pin="GND@1" pad="H2"/>
<connect gate="G$1" pin="GND@10" pad="J12"/>
<connect gate="G$1" pin="GND@11" pad="K2"/>
<connect gate="G$1" pin="GND@12" pad="K7"/>
<connect gate="G$1" pin="GND@13" pad="K8"/>
<connect gate="G$1" pin="GND@14" pad="K9"/>
<connect gate="G$1" pin="GND@15" pad="K10"/>
<connect gate="G$1" pin="GND@16" pad="K11"/>
<connect gate="G$1" pin="GND@17" pad="K12"/>
<connect gate="G$1" pin="GND@18" pad="L7"/>
<connect gate="G$1" pin="GND@19" pad="L8"/>
<connect gate="G$1" pin="GND@2" pad="H8"/>
<connect gate="G$1" pin="GND@20" pad="L9"/>
<connect gate="G$1" pin="GND@21" pad="L10"/>
<connect gate="G$1" pin="GND@22" pad="L11"/>
<connect gate="G$1" pin="GND@23" pad="M7"/>
<connect gate="G$1" pin="GND@24" pad="M9"/>
<connect gate="G$1" pin="GND@25" pad="M10"/>
<connect gate="G$1" pin="GND@3" pad="H10"/>
<connect gate="G$1" pin="GND@4" pad="H11"/>
<connect gate="G$1" pin="GND@5" pad="J7"/>
<connect gate="G$1" pin="GND@6" pad="J8"/>
<connect gate="G$1" pin="GND@7" pad="J9"/>
<connect gate="G$1" pin="GND@8" pad="J10"/>
<connect gate="G$1" pin="GND@9" pad="J11"/>
<connect gate="G$1" pin="MISO0" pad="T16"/>
<connect gate="G$1" pin="MISO1" pad="U18"/>
<connect gate="G$1" pin="MOSI0" pad="U16"/>
<connect gate="G$1" pin="MOSI1" pad="T17"/>
<connect gate="G$1" pin="NC@0" pad="A18"/>
<connect gate="G$1" pin="NC@1" pad="R3"/>
<connect gate="G$1" pin="NC@2" pad="V1"/>
<connect gate="G$1" pin="NC@3" pad="V18"/>
<connect gate="G$1" pin="NMI" pad="B11"/>
<connect gate="G$1" pin="PCI_AD0" pad="E17"/>
<connect gate="G$1" pin="PCI_AD1" pad="E18"/>
<connect gate="G$1" pin="PCI_AD10" pad="K18"/>
<connect gate="G$1" pin="PCI_AD11" pad="H16"/>
<connect gate="G$1" pin="PCI_AD12" pad="L18"/>
<connect gate="G$1" pin="PCI_AD13" pad="J17"/>
<connect gate="G$1" pin="PCI_AD14" pad="M18"/>
<connect gate="G$1" pin="PCI_AD15" pad="K17"/>
<connect gate="G$1" pin="PCI_AD16" pad="J16"/>
<connect gate="G$1" pin="PCI_AD17" pad="K16"/>
<connect gate="G$1" pin="PCI_AD18" pad="N18"/>
<connect gate="G$1" pin="PCI_AD19" pad="P18"/>
<connect gate="G$1" pin="PCI_AD2" pad="G16"/>
<connect gate="G$1" pin="PCI_AD20" pad="L17"/>
<connect gate="G$1" pin="PCI_AD21" pad="L16"/>
<connect gate="G$1" pin="PCI_AD22" pad="R18"/>
<connect gate="G$1" pin="PCI_AD23" pad="T18"/>
<connect gate="G$1" pin="PCI_AD24" pad="M17"/>
<connect gate="G$1" pin="PCI_AD25" pad="M16"/>
<connect gate="G$1" pin="PCI_AD26" pad="N17"/>
<connect gate="G$1" pin="PCI_AD27" pad="P17"/>
<connect gate="G$1" pin="PCI_AD28" pad="P15"/>
<connect gate="G$1" pin="PCI_AD29" pad="N16"/>
<connect gate="G$1" pin="PCI_AD3" pad="F17"/>
<connect gate="G$1" pin="PCI_AD30" pad="R17"/>
<connect gate="G$1" pin="PCI_AD31" pad="P16"/>
<connect gate="G$1" pin="PCI_AD4" pad="F18"/>
<connect gate="G$1" pin="PCI_AD5" pad="G18"/>
<connect gate="G$1" pin="PCI_AD6" pad="G17"/>
<connect gate="G$1" pin="PCI_AD7" pad="H18"/>
<connect gate="G$1" pin="PCI_AD8" pad="J18"/>
<connect gate="G$1" pin="PCI_AD9" pad="H17"/>
<connect gate="G$1" pin="PCI_CBE0" pad="F16"/>
<connect gate="G$1" pin="PCI_CBE1" pad="F15"/>
<connect gate="G$1" pin="PCI_CBE2" pad="E16"/>
<connect gate="G$1" pin="PCI_CBE3" pad="D17"/>
<connect gate="G$1" pin="PCI_CLK" pad="D14"/>
<connect gate="G$1" pin="PCI_DEVSEL" pad="C16"/>
<connect gate="G$1" pin="PCI_FRAME" pad="C17"/>
<connect gate="G$1" pin="PCI_GNT" pad="C18"/>
<connect gate="G$1" pin="PCI_IDSEL" pad="B18"/>
<connect gate="G$1" pin="PCI_INTA" pad="C14"/>
<connect gate="G$1" pin="PCI_INTB" pad="B15"/>
<connect gate="G$1" pin="PCI_INTC" pad="A15"/>
<connect gate="G$1" pin="PCI_INTD" pad="D13"/>
<connect gate="G$1" pin="PCI_IRDY" pad="E15"/>
<connect gate="G$1" pin="PCI_LOCK" pad="A16"/>
<connect gate="G$1" pin="PCI_PAR" pad="C15"/>
<connect gate="G$1" pin="PCI_PERR" pad="D15"/>
<connect gate="G$1" pin="PCI_REQ" pad="D16"/>
<connect gate="G$1" pin="PCI_RST" pad="D18"/>
<connect gate="G$1" pin="PCI_SERR" pad="B16"/>
<connect gate="G$1" pin="PCI_STOP" pad="A17"/>
<connect gate="G$1" pin="PCI_TRDY" pad="B17"/>
<connect gate="G$1" pin="PF0" pad="U8"/>
<connect gate="G$1" pin="PF1" pad="R8"/>
<connect gate="G$1" pin="PF10" pad="V12"/>
<connect gate="G$1" pin="PF11" pad="T12"/>
<connect gate="G$1" pin="PF12" pad="R12"/>
<connect gate="G$1" pin="PF13" pad="U12"/>
<connect gate="G$1" pin="PF14" pad="V13"/>
<connect gate="G$1" pin="PF15" pad="T13"/>
<connect gate="G$1" pin="PF2" pad="T8"/>
<connect gate="G$1" pin="PF3" pad="V10"/>
<connect gate="G$1" pin="PF4" pad="U9"/>
<connect gate="G$1" pin="PF5" pad="R9"/>
<connect gate="G$1" pin="PF6" pad="T9"/>
<connect gate="G$1" pin="PF7" pad="R11"/>
<connect gate="G$1" pin="PF8" pad="T11"/>
<connect gate="G$1" pin="PF9" pad="U11"/>
<connect gate="G$1" pin="RESET_B" pad="B9"/>
<connect gate="G$1" pin="RFS0" pad="U13"/>
<connect gate="G$1" pin="RFS1" pad="V16"/>
<connect gate="G$1" pin="RSCLK0" pad="R13"/>
<connect gate="G$1" pin="RSCLK1" pad="U14"/>
<connect gate="G$1" pin="RX0" pad="A7"/>
<connect gate="G$1" pin="RX1" pad="B8"/>
<connect gate="G$1" pin="SA10" pad="M1"/>
<connect gate="G$1" pin="SCAS_B" pad="L3"/>
<connect gate="G$1" pin="SCK0" pad="U17"/>
<connect gate="G$1" pin="SCK1" pad="R16"/>
<connect gate="G$1" pin="SCKE" pad="L1"/>
<connect gate="G$1" pin="SCLK0" pad="K1"/>
<connect gate="G$1" pin="SLEEP" pad="D12"/>
<connect gate="G$1" pin="SMS_B0" pad="M2"/>
<connect gate="G$1" pin="SMS_B1" pad="P1"/>
<connect gate="G$1" pin="SMS_B2" pad="N1"/>
<connect gate="G$1" pin="SMS_B3" pad="K3"/>
<connect gate="G$1" pin="SRAS_B" pad="L2"/>
<connect gate="G$1" pin="SUSPEND" pad="A11"/>
<connect gate="G$1" pin="SWE_B" pad="J3"/>
<connect gate="G$1" pin="TCK" pad="D10"/>
<connect gate="G$1" pin="TDI" pad="C11"/>
<connect gate="G$1" pin="TDO" pad="D11"/>
<connect gate="G$1" pin="TFS0" pad="T14"/>
<connect gate="G$1" pin="TFS1" pad="R15"/>
<connect gate="G$1" pin="TMR0" pad="B7"/>
<connect gate="G$1" pin="TMR1" pad="C7"/>
<connect gate="G$1" pin="TMR2" pad="D7"/>
<connect gate="G$1" pin="TMS" pad="A12"/>
<connect gate="G$1" pin="TRST_B" pad="B12"/>
<connect gate="G$1" pin="TSCLK0" pad="V15"/>
<connect gate="G$1" pin="TSCLK1" pad="T15"/>
<connect gate="G$1" pin="TX0" pad="A8"/>
<connect gate="G$1" pin="TX1" pad="C8"/>
<connect gate="G$1" pin="TXDMNS" pad="G10"/>
<connect gate="G$1" pin="TXDPLS" pad="B10"/>
<connect gate="G$1" pin="TXEN" pad="C10"/>
<connect gate="G$1" pin="USB_CLK" pad="G7"/>
<connect gate="G$1" pin="VDDEXT@0" pad="E4"/>
<connect gate="G$1" pin="VDDEXT@1" pad="G4"/>
<connect gate="G$1" pin="VDDEXT@2" pad="G8"/>
<connect gate="G$1" pin="VDDEXT@3" pad="J1"/>
<connect gate="G$1" pin="VDDEXT@4" pad="J2"/>
<connect gate="G$1" pin="VDDEXT@5" pad="J4"/>
<connect gate="G$1" pin="VDDEXT@6" pad="K4"/>
<connect gate="G$1" pin="VDDEXT@7" pad="L4"/>
<connect gate="G$1" pin="VDDEXT@8" pad="M4"/>
<connect gate="G$1" pin="VDDEXT@9" pad="P4"/>
<connect gate="G$1" pin="VDDINT@0" pad="F4"/>
<connect gate="G$1" pin="VDDINT@1" pad="G11"/>
<connect gate="G$1" pin="VDDINT@10" pad="M12"/>
<connect gate="G$1" pin="VDDINT@11" pad="N4"/>
<connect gate="G$1" pin="VDDINT@12" pad="N15"/>
<connect gate="G$1" pin="VDDINT@2" pad="G12"/>
<connect gate="G$1" pin="VDDINT@3" pad="G15"/>
<connect gate="G$1" pin="VDDINT@4" pad="H4"/>
<connect gate="G$1" pin="VDDINT@5" pad="H9"/>
<connect gate="G$1" pin="VDDINT@6" pad="H12"/>
<connect gate="G$1" pin="VDDINT@7" pad="L12"/>
<connect gate="G$1" pin="VDDINT@8" pad="M8"/>
<connect gate="G$1" pin="VDDINT@9" pad="M11"/>
<connect gate="G$1" pin="VDDPCIEXT@0" pad="H15"/>
<connect gate="G$1" pin="VDDPCIEXT@1" pad="J15"/>
<connect gate="G$1" pin="VDDPCIEXT@2" pad="K15"/>
<connect gate="G$1" pin="VDDPCIEXT@3" pad="L15"/>
<connect gate="G$1" pin="VDDPCIEXT@4" pad="M15"/>
<connect gate="G$1" pin="VDDPLL" pad="G9"/>
<connect gate="G$1" pin="VDDRTC" pad="U10"/>
<connect gate="G$1" pin="VSSPLL" pad="A10"/>
<connect gate="G$1" pin="VSSRTC" pad="V11"/>
<connect gate="G$1" pin="XTALI" pad="R10"/>
<connect gate="G$1" pin="XTALO" pad="T10"/>
<connect gate="G$1" pin="XVER_DATA" pad="A9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1439074"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD6624A" prefix="IC">
<description>&lt;b&gt;Four-Channel, 100 MSPS Digital Receive Signal Processor (RSP)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 11&lt;/i&gt;&lt;br&gt;
Source: 90033586AD6624A.bsdl.txt&lt;br&gt;
http://www.analog.com/UploadedFiles/Data_Sheets/171976900AD6624A_0.pdf</description>
<gates>
<gate name="G$1" symbol="AD6624A"/>
</gates>
<devices>
<device name="" package="PBGA196">
<connects>
<connect gate="G$1" pin="A0" pad="M10"/>
<connect gate="G$1" pin="A1" pad="P11"/>
<connect gate="G$1" pin="A2" pad="N10"/>
<connect gate="G$1" pin="CHIP_ID0" pad="K14"/>
<connect gate="G$1" pin="CHIP_ID1" pad="K12"/>
<connect gate="G$1" pin="CHIP_ID2" pad="L14"/>
<connect gate="G$1" pin="CHIP_ID3" pad="K13"/>
<connect gate="G$1" pin="CLK" pad="E1"/>
<connect gate="G$1" pin="CS" pad="N11"/>
<connect gate="G$1" pin="D0" pad="P9"/>
<connect gate="G$1" pin="D1" pad="N8"/>
<connect gate="G$1" pin="D2" pad="M7"/>
<connect gate="G$1" pin="D3" pad="P8"/>
<connect gate="G$1" pin="D4" pad="N7"/>
<connect gate="G$1" pin="D5" pad="M6"/>
<connect gate="G$1" pin="D6" pad="P6"/>
<connect gate="G$1" pin="D7" pad="N6"/>
<connect gate="G$1" pin="DR0" pad="F13"/>
<connect gate="G$1" pin="DR1" pad="D13"/>
<connect gate="G$1" pin="DR2" pad="A11"/>
<connect gate="G$1" pin="DR3" pad="B8"/>
<connect gate="G$1" pin="DS" pad="M8"/>
<connect gate="G$1" pin="DTACK" pad="N9"/>
<connect gate="G$1" pin="EXPA0" pad="F2"/>
<connect gate="G$1" pin="EXPA1" pad="F1"/>
<connect gate="G$1" pin="EXPA2" pad="F3"/>
<connect gate="G$1" pin="EXPB0" pad="A8"/>
<connect gate="G$1" pin="EXPB1" pad="A7"/>
<connect gate="G$1" pin="EXPB2" pad="C8"/>
<connect gate="G$1" pin="IENA" pad="M1"/>
<connect gate="G$1" pin="IENB" pad="E2"/>
<connect gate="G$1" pin="INA0" pad="K3"/>
<connect gate="G$1" pin="INA1" pad="L1"/>
<connect gate="G$1" pin="INA10" pad="G3"/>
<connect gate="G$1" pin="INA11" pad="H1"/>
<connect gate="G$1" pin="INA12" pad="G1"/>
<connect gate="G$1" pin="INA13" pad="G2"/>
<connect gate="G$1" pin="INA2" pad="K2"/>
<connect gate="G$1" pin="INA3" pad="L3"/>
<connect gate="G$1" pin="INA4" pad="J3"/>
<connect gate="G$1" pin="INA5" pad="K1"/>
<connect gate="G$1" pin="INA6" pad="J2"/>
<connect gate="G$1" pin="INA7" pad="H3"/>
<connect gate="G$1" pin="INA8" pad="J1"/>
<connect gate="G$1" pin="INA9" pad="H2"/>
<connect gate="G$1" pin="INB0" pad="D3"/>
<connect gate="G$1" pin="INB1" pad="C1"/>
<connect gate="G$1" pin="INB10" pad="B6"/>
<connect gate="G$1" pin="INB11" pad="C7"/>
<connect gate="G$1" pin="INB12" pad="A6"/>
<connect gate="G$1" pin="INB13" pad="B7"/>
<connect gate="G$1" pin="INB2" pad="D2"/>
<connect gate="G$1" pin="INB3" pad="B1"/>
<connect gate="G$1" pin="INB4" pad="B4"/>
<connect gate="G$1" pin="INB5" pad="A3"/>
<connect gate="G$1" pin="INB6" pad="A4"/>
<connect gate="G$1" pin="INB7" pad="B5"/>
<connect gate="G$1" pin="INB8" pad="C4"/>
<connect gate="G$1" pin="INB9" pad="C6"/>
<connect gate="G$1" pin="LIA_A" pad="N4"/>
<connect gate="G$1" pin="LIA_B" pad="P2"/>
<connect gate="G$1" pin="LIB_A" pad="E3"/>
<connect gate="G$1" pin="LIB_B" pad="D1"/>
<connect gate="G$1" pin="MODE" pad="M11"/>
<connect gate="G$1" pin="RESET" pad="P5"/>
<connect gate="G$1" pin="R_W" pad="P10"/>
<connect gate="G$1" pin="SBM0" pad="J13"/>
<connect gate="G$1" pin="SCLK0" pad="G14"/>
<connect gate="G$1" pin="SCLK1" pad="F12"/>
<connect gate="G$1" pin="SCLK2" pad="C12"/>
<connect gate="G$1" pin="SCLK3" pad="C10"/>
<connect gate="G$1" pin="SDFE0" pad="G12"/>
<connect gate="G$1" pin="SDFE1" pad="C14"/>
<connect gate="G$1" pin="SDFE2" pad="B10"/>
<connect gate="G$1" pin="SDFE3" pad="C9"/>
<connect gate="G$1" pin="SDFS0" pad="H12"/>
<connect gate="G$1" pin="SDFS1" pad="D12"/>
<connect gate="G$1" pin="SDFS2" pad="A13"/>
<connect gate="G$1" pin="SDFS3" pad="A10"/>
<connect gate="G$1" pin="SDIN0" pad="F14"/>
<connect gate="G$1" pin="SDIN1" pad="D14"/>
<connect gate="G$1" pin="SDIN2" pad="C11"/>
<connect gate="G$1" pin="SDIN3" pad="A9"/>
<connect gate="G$1" pin="SDIV0" pad="H14"/>
<connect gate="G$1" pin="SDIV1" pad="H13"/>
<connect gate="G$1" pin="SDIV2" pad="J12"/>
<connect gate="G$1" pin="SDIV3" pad="J14"/>
<connect gate="G$1" pin="SDO0" pad="G13"/>
<connect gate="G$1" pin="SDO1" pad="E13"/>
<connect gate="G$1" pin="SDO2" pad="B11"/>
<connect gate="G$1" pin="SDO3" pad="B9"/>
<connect gate="G$1" pin="SYNCA" pad="M5"/>
<connect gate="G$1" pin="SYNCB" pad="P4"/>
<connect gate="G$1" pin="SYNCC" pad="N5"/>
<connect gate="G$1" pin="SYNCD" pad="M4"/>
<connect gate="G$1" pin="TCLK" pad="N14"/>
<connect gate="G$1" pin="TDI" pad="L12"/>
<connect gate="G$1" pin="TDO" pad="M14"/>
<connect gate="G$1" pin="TMS" pad="L13"/>
<connect gate="G$1" pin="TRST" pad="M12"/>
<connect gate="G$1" pin="VDDCORE@1" pad="E6"/>
<connect gate="G$1" pin="VDDCORE@10" pad="K9"/>
<connect gate="G$1" pin="VDDCORE@2" pad="E8"/>
<connect gate="G$1" pin="VDDCORE@3" pad="E10"/>
<connect gate="G$1" pin="VDDCORE@4" pad="F5"/>
<connect gate="G$1" pin="VDDCORE@5" pad="G10"/>
<connect gate="G$1" pin="VDDCORE@6" pad="H5"/>
<connect gate="G$1" pin="VDDCORE@7" pad="J10"/>
<connect gate="G$1" pin="VDDCORE@8" pad="K5"/>
<connect gate="G$1" pin="VDDCORE@9" pad="K7"/>
<connect gate="G$1" pin="VDDRING@1" pad="E5"/>
<connect gate="G$1" pin="VDDRING@10" pad="K10"/>
<connect gate="G$1" pin="VDDRING@2" pad="E7"/>
<connect gate="G$1" pin="VDDRING@3" pad="E9"/>
<connect gate="G$1" pin="VDDRING@4" pad="F10"/>
<connect gate="G$1" pin="VDDRING@5" pad="G5"/>
<connect gate="G$1" pin="VDDRING@6" pad="H10"/>
<connect gate="G$1" pin="VDDRING@7" pad="J5"/>
<connect gate="G$1" pin="VDDRING@8" pad="K6"/>
<connect gate="G$1" pin="VDDRING@9" pad="K8"/>
<connect gate="G$1" pin="VSSCORE" pad="F6"/>
<connect gate="G$1" pin="VSSCORE@1" pad="F7"/>
<connect gate="G$1" pin="VSSCORE@2" pad="F8"/>
<connect gate="G$1" pin="VSSCORE@3" pad="F9"/>
<connect gate="G$1" pin="VSSCORE@4" pad="G6"/>
<connect gate="G$1" pin="VSSCORE@5" pad="G7"/>
<connect gate="G$1" pin="VSSCORE@6" pad="G8"/>
<connect gate="G$1" pin="VSSCORE@7" pad="G9"/>
<connect gate="G$1" pin="VSSRING@1" pad="H6"/>
<connect gate="G$1" pin="VSSRING@2" pad="H7"/>
<connect gate="G$1" pin="VSSRING@3" pad="H8"/>
<connect gate="G$1" pin="VSSRING@4" pad="H9"/>
<connect gate="G$1" pin="VSSRING@5" pad="J6"/>
<connect gate="G$1" pin="VSSRING@6" pad="J7"/>
<connect gate="G$1" pin="VSSRING@7" pad="J8"/>
<connect gate="G$1" pin="VSSRING@8" pad="J9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD6624AABC"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="94C0338"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC70*" prefix="IC">
<description>&lt;b&gt;Precision Analog Microcontroller 12-bit Analog I/O, ARM7TDMI® MCU&lt;/b&gt;&lt;p&gt;
ADuC7019/ADuC7020&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/288945048AD7C7019_20_1_2_4_5_6_7_0.pdf</description>
<gates>
<gate name="G$1" symbol="ADUC7019"/>
</gates>
<devices>
<device name="" package="LFCSP40">
<connects>
<connect gate="G$1" pin="!RST" pad="19"/>
<connect gate="G$1" pin="ADC0" pad="38"/>
<connect gate="G$1" pin="ADC1" pad="39"/>
<connect gate="G$1" pin="ADC2/CMP0" pad="40"/>
<connect gate="G$1" pin="ADC3/CMP1" pad="1"/>
<connect gate="G$1" pin="ADC4" pad="2"/>
<connect gate="G$1" pin="AGND" pad="36"/>
<connect gate="G$1" pin="AVDD" pad="37"/>
<connect gate="G$1" pin="DAC0/ADC12" pad="4"/>
<connect gate="G$1" pin="DAC1/ADC13" pad="5"/>
<connect gate="G$1" pin="DAC2/ADC14" pad="6"/>
<connect gate="G$1" pin="DAC3/ADC15" pad="7"/>
<connect gate="G$1" pin="DGND" pad="17"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GNDREF" pad="3"/>
<connect gate="G$1" pin="IOGND" pad="14"/>
<connect gate="G$1" pin="IOVDD" pad="15"/>
<connect gate="G$1" pin="LVDD" pad="16"/>
<connect gate="G$1" pin="P0.0/BM/CMPOUT/MS2" pad="10"/>
<connect gate="G$1" pin="P0.3/TRST/A16" pad="18"/>
<connect gate="G$1" pin="P0.4/IRQ0" pad="20"/>
<connect gate="G$1" pin="P0.5/IRQ1" pad="21"/>
<connect gate="G$1" pin="P0.6/T1/MRST/AE" pad="11"/>
<connect gate="G$1" pin="P0.7/ECLK/XCLK" pad="23"/>
<connect gate="G$1" pin="P1.0/T1/SPM0" pad="33"/>
<connect gate="G$1" pin="P1.1/SPM1" pad="32"/>
<connect gate="G$1" pin="P1.2/SPM2" pad="31"/>
<connect gate="G$1" pin="P1.3/SPM3" pad="30"/>
<connect gate="G$1" pin="P1.4/SPM4/IRQ2" pad="29"/>
<connect gate="G$1" pin="P1.5/SPM5/IRQ3" pad="28"/>
<connect gate="G$1" pin="P1.6/SPM6" pad="27"/>
<connect gate="G$1" pin="P1.7/SPM7" pad="26"/>
<connect gate="G$1" pin="P2.0/SPM9/!CONVSTART" pad="22"/>
<connect gate="G$1" pin="P4.2" pad="34"/>
<connect gate="G$1" pin="TCK" pad="12"/>
<connect gate="G$1" pin="TDI" pad="9"/>
<connect gate="G$1" pin="TDO" pad="13"/>
<connect gate="G$1" pin="TMS" pad="8"/>
<connect gate="G$1" pin="VREF" pad="35"/>
<connect gate="G$1" pin="XCLKI" pad="25"/>
<connect gate="G$1" pin="XCLKO" pad="24"/>
</connects>
<technologies>
<technology name="19BCPZ62I">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7019BCPZ62I"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="19M0734"/>
</technology>
<technology name="19BCPZ62I-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7019BCPZ62IRL7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8312"/>
</technology>
<technology name="19BCPZ62IRL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7019BCPZ62IRL7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8312"/>
</technology>
<technology name="20BCPZ62">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7020BCPZ62"/>
<attribute name="OC_FARNELL" value="1162634"/>
<attribute name="OC_NEWARK" value="19M0735"/>
</technology>
<technology name="20BCPZ62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7020BCPZ62-RL7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8315"/>
</technology>
<technology name="20BCPZ62-RL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="20BCPZ62I">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7020BCPZ62I"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="61M4009"/>
</technology>
<technology name="20BCPZ62I-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7020BCPZ62I-RL"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8316"/>
</technology>
<technology name="20BCPZ62IRL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7020BCPZ62IRL7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8317"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC7021*" prefix="IC">
<description>&lt;b&gt;Precision Analog Microcontroller 12-bit Analog I/O, ARM7TDMI® MCU&lt;/b&gt;&lt;p&gt;
ADuC7021&lt;br&gt;
Source: Source: http://www.analog.com/UploadedFiles/Data_Sheets/288945048AD7C7019_20_1_2_4_5_6_7_0.pdf</description>
<gates>
<gate name="G$1" symbol="ADUC7021"/>
</gates>
<devices>
<device name="" package="LFCSP40">
<connects>
<connect gate="G$1" pin="!RST" pad="19"/>
<connect gate="G$1" pin="ADC0" pad="37"/>
<connect gate="G$1" pin="ADC1" pad="38"/>
<connect gate="G$1" pin="ADC2/CMP0" pad="39"/>
<connect gate="G$1" pin="ADC3/CMP1" pad="40"/>
<connect gate="G$1" pin="ADC4" pad="1"/>
<connect gate="G$1" pin="ADC5" pad="2"/>
<connect gate="G$1" pin="ADC6" pad="3"/>
<connect gate="G$1" pin="ADC7" pad="4"/>
<connect gate="G$1" pin="AGND" pad="35"/>
<connect gate="G$1" pin="AVDD" pad="36"/>
<connect gate="G$1" pin="DAC0/ADC12" pad="6"/>
<connect gate="G$1" pin="DAC1/ADC13" pad="7"/>
<connect gate="G$1" pin="DGND" pad="17"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GNDREF" pad="5"/>
<connect gate="G$1" pin="IOGND" pad="14"/>
<connect gate="G$1" pin="IOVDD" pad="15"/>
<connect gate="G$1" pin="LVDD" pad="16"/>
<connect gate="G$1" pin="P0.0/BM/CMPOUT" pad="10"/>
<connect gate="G$1" pin="P0.3/TRST/A16" pad="18"/>
<connect gate="G$1" pin="P0.4/IRQ0" pad="20"/>
<connect gate="G$1" pin="P0.5/IRQ1" pad="21"/>
<connect gate="G$1" pin="P0.6/T1/MRST/AE" pad="11"/>
<connect gate="G$1" pin="P0.7/ECLK/XCLK" pad="23"/>
<connect gate="G$1" pin="P1.0/T1/SPM0" pad="33"/>
<connect gate="G$1" pin="P1.1/SPM1" pad="32"/>
<connect gate="G$1" pin="P1.2/SPM2" pad="31"/>
<connect gate="G$1" pin="P1.3/SPM3" pad="30"/>
<connect gate="G$1" pin="P1.4/SPM4/IRQ2" pad="29"/>
<connect gate="G$1" pin="P1.5/SPM5/IRQ3" pad="28"/>
<connect gate="G$1" pin="P1.6/SPM6" pad="27"/>
<connect gate="G$1" pin="P1.7/SPM7" pad="26"/>
<connect gate="G$1" pin="P2.0/SPM9/!CONVSTART" pad="22"/>
<connect gate="G$1" pin="TCK" pad="12"/>
<connect gate="G$1" pin="TDI" pad="9"/>
<connect gate="G$1" pin="TDO" pad="13"/>
<connect gate="G$1" pin="TMS" pad="8"/>
<connect gate="G$1" pin="VREF" pad="34"/>
<connect gate="G$1" pin="XCLKI" pad="25"/>
<connect gate="G$1" pin="XCLKO" pad="24"/>
</connects>
<technologies>
<technology name="BCPZ32">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7021BCPZ32"/>
<attribute name="OC_FARNELL" value="1274142"/>
<attribute name="OC_NEWARK" value="31M3910"/>
</technology>
<technology name="BCPZ32-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="BCPZ32-RL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="BCPZ62">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7021BCPZ62"/>
<attribute name="OC_FARNELL" value="1162635"/>
<attribute name="OC_NEWARK" value="31M3911"/>
</technology>
<technology name="BCPZ62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="BCPZ62-RL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="BCPZ62I">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7021BCPZ62I"/>
<attribute name="OC_FARNELL" value="1162636"/>
<attribute name="OC_NEWARK" value="19M0738"/>
</technology>
<technology name="BCPZ62I-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="BCPZ62IRL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC7022*" prefix="IC">
<description>&lt;b&gt;Precision Analog Microcontroller 12-bit Analog I/O, ARM7TDMI® MCU&lt;/b&gt;&lt;p&gt;
ADuC7022&lt;br&gt;
Source: Source: http://www.analog.com/UploadedFiles/Data_Sheets/288945048AD7C7019_20_1_2_4_5_6_7_0.pdf</description>
<gates>
<gate name="G$1" symbol="ADUC7022"/>
</gates>
<devices>
<device name="" package="LFCSP40">
<connects>
<connect gate="G$1" pin="!RST" pad="18"/>
<connect gate="G$1" pin="ADC0" pad="36"/>
<connect gate="G$1" pin="ADC1" pad="37"/>
<connect gate="G$1" pin="ADC2/CMP0" pad="38"/>
<connect gate="G$1" pin="ADC3/CMP1" pad="39"/>
<connect gate="G$1" pin="ADC4" pad="40"/>
<connect gate="G$1" pin="ADC5" pad="1"/>
<connect gate="G$1" pin="ADC6" pad="2"/>
<connect gate="G$1" pin="ADC7" pad="3"/>
<connect gate="G$1" pin="ADC8" pad="4"/>
<connect gate="G$1" pin="ADC9" pad="5"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AVDD" pad="35"/>
<connect gate="G$1" pin="DGND" pad="16"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GNDREF" pad="6"/>
<connect gate="G$1" pin="IOGND" pad="13"/>
<connect gate="G$1" pin="IOVDD" pad="14"/>
<connect gate="G$1" pin="LVDD" pad="15"/>
<connect gate="G$1" pin="P0.0/BM/CMPOUT/MS2" pad="9"/>
<connect gate="G$1" pin="P0.3/TRST/A16" pad="17"/>
<connect gate="G$1" pin="P0.4/IRQ0" pad="19"/>
<connect gate="G$1" pin="P0.5/IRQ1" pad="20"/>
<connect gate="G$1" pin="P0.6/T1/MRST/AE" pad="10"/>
<connect gate="G$1" pin="P0.7/ECLK/XCLK" pad="22"/>
<connect gate="G$1" pin="P1.0/T1/SPM0" pad="32"/>
<connect gate="G$1" pin="P1.1/SPM1" pad="31"/>
<connect gate="G$1" pin="P1.2/SPM2" pad="30"/>
<connect gate="G$1" pin="P1.3/SPM3" pad="29"/>
<connect gate="G$1" pin="P1.4/SPM4/IRQ2" pad="28"/>
<connect gate="G$1" pin="P1.5/SPM5/IRQ3" pad="27"/>
<connect gate="G$1" pin="P1.6/SPM6" pad="26"/>
<connect gate="G$1" pin="P1.7/SPM7" pad="25"/>
<connect gate="G$1" pin="P2.0/SPM9/!CONVSTART" pad="21"/>
<connect gate="G$1" pin="TCK" pad="11"/>
<connect gate="G$1" pin="TDI" pad="8"/>
<connect gate="G$1" pin="TDO" pad="12"/>
<connect gate="G$1" pin="TMS" pad="7"/>
<connect gate="G$1" pin="VREF" pad="33"/>
<connect gate="G$1" pin="XCLKI" pad="24"/>
<connect gate="G$1" pin="XCLKO" pad="23"/>
</connects>
<technologies>
<technology name="BCPZ32">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7022BCPZ32"/>
<attribute name="OC_FARNELL" value="1162638"/>
<attribute name="OC_NEWARK" value="19M0739"/>
</technology>
<technology name="BCPZ32-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="BCPZ32-RL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="BCPZ62">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7022BCPZ62"/>
<attribute name="OC_FARNELL" value="1162637"/>
<attribute name="OC_NEWARK" value="19M0740"/>
</technology>
<technology name="BCPZ62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="BCPZ62-RL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC702?*" prefix="IC">
<description>&lt;b&gt;Precision Analog Microcontroller 12-bit Analog I/O, ARM7TDMI® MCU&lt;/b&gt;&lt;p&gt;
ADuC7022/24&lt;br&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/288945048AD7C7019_20_1_2_4_5_6_7_0.pdf</description>
<gates>
<gate name="G$1" symbol="ADUC7024"/>
</gates>
<devices>
<device name="4BCPZ" package="LFCSP64">
<connects>
<connect gate="G$1" pin="!RST" pad="28"/>
<connect gate="G$1" pin="ADC0" pad="61"/>
<connect gate="G$1" pin="ADC1" pad="62"/>
<connect gate="G$1" pin="ADC2/CMP0" pad="63"/>
<connect gate="G$1" pin="ADC3/CMP1" pad="64"/>
<connect gate="G$1" pin="ADC4" pad="1"/>
<connect gate="G$1" pin="ADC5" pad="2"/>
<connect gate="G$1" pin="ADC6" pad="3"/>
<connect gate="G$1" pin="ADC7" pad="4"/>
<connect gate="G$1" pin="ADC8" pad="5"/>
<connect gate="G$1" pin="ADC9" pad="6"/>
<connect gate="G$1" pin="ADCNEG" pad="8"/>
<connect gate="G$1" pin="AGND" pad="58"/>
<connect gate="G$1" pin="AVDD" pad="59"/>
<connect gate="G$1" pin="DAC0/ADC12" pad="9"/>
<connect gate="G$1" pin="DAC1/ADC13" pad="10"/>
<connect gate="G$1" pin="DACGND" pad="57"/>
<connect gate="G$1" pin="DACREF" pad="56"/>
<connect gate="G$1" pin="DACVDD" pad="60"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="GNDREF" pad="7"/>
<connect gate="G$1" pin="IOGND" pad="19"/>
<connect gate="G$1" pin="IOGND@1" pad="41"/>
<connect gate="G$1" pin="IOVDD" pad="20"/>
<connect gate="G$1" pin="IOVDD@1" pad="42"/>
<connect gate="G$1" pin="LVDD" pad="21"/>
<connect gate="G$1" pin="P0.0/BM/CMPOUT/MS2" pad="15"/>
<connect gate="G$1" pin="P0.3/TRST/A16" pad="27"/>
<connect gate="G$1" pin="P0.4/IRQ0" pad="31"/>
<connect gate="G$1" pin="P0.5/IRQ1" pad="32"/>
<connect gate="G$1" pin="P0.6/T1/MRST/AE" pad="16"/>
<connect gate="G$1" pin="P0.7/ECLK/XCLK" pad="34"/>
<connect gate="G$1" pin="P1.0/T1/SPM0" pad="50"/>
<connect gate="G$1" pin="P1.1/SPM1" pad="49"/>
<connect gate="G$1" pin="P1.2/SPM2" pad="48"/>
<connect gate="G$1" pin="P1.3/SPM3" pad="47"/>
<connect gate="G$1" pin="P1.4/SPM4/IRQ2" pad="46"/>
<connect gate="G$1" pin="P1.5/SPM5/IRQ3" pad="45"/>
<connect gate="G$1" pin="P1.6/SPM6" pad="40"/>
<connect gate="G$1" pin="P1.7/SPM7" pad="39"/>
<connect gate="G$1" pin="P2.0/SPM9/!CONVSTART" pad="33"/>
<connect gate="G$1" pin="P3.0/AD0/PWM0H" pad="23"/>
<connect gate="G$1" pin="P3.1/AD1/PWM0L" pad="24"/>
<connect gate="G$1" pin="P3.2/AD2/PWM1H" pad="25"/>
<connect gate="G$1" pin="P3.3/AD3/PWM1L" pad="26"/>
<connect gate="G$1" pin="P3.4/AD4/PWM2H" pad="29"/>
<connect gate="G$1" pin="P3.5/AD5/PWM2L" pad="30"/>
<connect gate="G$1" pin="P3.6/AD6/PWMTRIP" pad="37"/>
<connect gate="G$1" pin="P3.7/AD7/PWMSYNC" pad="38"/>
<connect gate="G$1" pin="P4.0/AD8" pad="43"/>
<connect gate="G$1" pin="P4.1/AD9" pad="44"/>
<connect gate="G$1" pin="P4.2/AD10" pad="51"/>
<connect gate="G$1" pin="P4.3/AD11" pad="52"/>
<connect gate="G$1" pin="P4.4/AD12" pad="53"/>
<connect gate="G$1" pin="P4.5/AD13" pad="54"/>
<connect gate="G$1" pin="P4.6/AD14" pad="13"/>
<connect gate="G$1" pin="P4.7/AD15" pad="14"/>
<connect gate="G$1" pin="TCK" pad="17"/>
<connect gate="G$1" pin="TDI" pad="12"/>
<connect gate="G$1" pin="TDO" pad="18"/>
<connect gate="G$1" pin="TMS" pad="11"/>
<connect gate="G$1" pin="VREF" pad="55"/>
<connect gate="G$1" pin="XCLKI" pad="36"/>
<connect gate="G$1" pin="XCLKO" pad="35"/>
</connects>
<technologies>
<technology name="62">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="62-RL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="4BSTZ" package="LQFP-ST-64-2">
<connects>
<connect gate="G$1" pin="!RST" pad="28"/>
<connect gate="G$1" pin="ADC0" pad="61"/>
<connect gate="G$1" pin="ADC1" pad="62"/>
<connect gate="G$1" pin="ADC2/CMP0" pad="63"/>
<connect gate="G$1" pin="ADC3/CMP1" pad="64"/>
<connect gate="G$1" pin="ADC4" pad="1"/>
<connect gate="G$1" pin="ADC5" pad="2"/>
<connect gate="G$1" pin="ADC6" pad="3"/>
<connect gate="G$1" pin="ADC7" pad="4"/>
<connect gate="G$1" pin="ADC8" pad="5"/>
<connect gate="G$1" pin="ADC9" pad="6"/>
<connect gate="G$1" pin="ADCNEG" pad="8"/>
<connect gate="G$1" pin="AGND" pad="58"/>
<connect gate="G$1" pin="AVDD" pad="59"/>
<connect gate="G$1" pin="DAC0/ADC12" pad="9"/>
<connect gate="G$1" pin="DAC1/ADC13" pad="10"/>
<connect gate="G$1" pin="DACGND" pad="57"/>
<connect gate="G$1" pin="DACREF" pad="56"/>
<connect gate="G$1" pin="DACVDD" pad="60"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="GNDREF" pad="7"/>
<connect gate="G$1" pin="IOGND" pad="19"/>
<connect gate="G$1" pin="IOGND@1" pad="41"/>
<connect gate="G$1" pin="IOVDD" pad="20"/>
<connect gate="G$1" pin="IOVDD@1" pad="42"/>
<connect gate="G$1" pin="LVDD" pad="21"/>
<connect gate="G$1" pin="P0.0/BM/CMPOUT/MS2" pad="15"/>
<connect gate="G$1" pin="P0.3/TRST/A16" pad="27"/>
<connect gate="G$1" pin="P0.4/IRQ0" pad="31"/>
<connect gate="G$1" pin="P0.5/IRQ1" pad="32"/>
<connect gate="G$1" pin="P0.6/T1/MRST/AE" pad="16"/>
<connect gate="G$1" pin="P0.7/ECLK/XCLK" pad="34"/>
<connect gate="G$1" pin="P1.0/T1/SPM0" pad="50"/>
<connect gate="G$1" pin="P1.1/SPM1" pad="49"/>
<connect gate="G$1" pin="P1.2/SPM2" pad="48"/>
<connect gate="G$1" pin="P1.3/SPM3" pad="47"/>
<connect gate="G$1" pin="P1.4/SPM4/IRQ2" pad="46"/>
<connect gate="G$1" pin="P1.5/SPM5/IRQ3" pad="45"/>
<connect gate="G$1" pin="P1.6/SPM6" pad="40"/>
<connect gate="G$1" pin="P1.7/SPM7" pad="39"/>
<connect gate="G$1" pin="P2.0/SPM9/!CONVSTART" pad="33"/>
<connect gate="G$1" pin="P3.0/AD0/PWM0H" pad="23"/>
<connect gate="G$1" pin="P3.1/AD1/PWM0L" pad="24"/>
<connect gate="G$1" pin="P3.2/AD2/PWM1H" pad="25"/>
<connect gate="G$1" pin="P3.3/AD3/PWM1L" pad="26"/>
<connect gate="G$1" pin="P3.4/AD4/PWM2H" pad="29"/>
<connect gate="G$1" pin="P3.5/AD5/PWM2L" pad="30"/>
<connect gate="G$1" pin="P3.6/AD6/PWMTRIP" pad="37"/>
<connect gate="G$1" pin="P3.7/AD7/PWMSYNC" pad="38"/>
<connect gate="G$1" pin="P4.0/AD8" pad="43"/>
<connect gate="G$1" pin="P4.1/AD9" pad="44"/>
<connect gate="G$1" pin="P4.2/AD10" pad="51"/>
<connect gate="G$1" pin="P4.3/AD11" pad="52"/>
<connect gate="G$1" pin="P4.4/AD12" pad="53"/>
<connect gate="G$1" pin="P4.5/AD13" pad="54"/>
<connect gate="G$1" pin="P4.6/AD14" pad="13"/>
<connect gate="G$1" pin="P4.7/AD15" pad="14"/>
<connect gate="G$1" pin="TCK" pad="17"/>
<connect gate="G$1" pin="TDI" pad="12"/>
<connect gate="G$1" pin="TDO" pad="18"/>
<connect gate="G$1" pin="TMS" pad="11"/>
<connect gate="G$1" pin="VREF" pad="55"/>
<connect gate="G$1" pin="XCLKI" pad="36"/>
<connect gate="G$1" pin="XCLKO" pad="35"/>
</connects>
<technologies>
<technology name="62">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7024BSTZ62-RL"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8337"/>
</technology>
<technology name="62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5BCPZ" package="LFCSP64">
<connects>
<connect gate="G$1" pin="!RST" pad="28"/>
<connect gate="G$1" pin="ADC0" pad="61"/>
<connect gate="G$1" pin="ADC1" pad="62"/>
<connect gate="G$1" pin="ADC2/CMP0" pad="63"/>
<connect gate="G$1" pin="ADC3/CMP1" pad="64"/>
<connect gate="G$1" pin="ADC4" pad="1"/>
<connect gate="G$1" pin="ADC5" pad="2"/>
<connect gate="G$1" pin="ADC6" pad="3"/>
<connect gate="G$1" pin="ADC7" pad="4"/>
<connect gate="G$1" pin="ADC8" pad="5"/>
<connect gate="G$1" pin="ADC9" pad="6"/>
<connect gate="G$1" pin="ADCNEG" pad="8"/>
<connect gate="G$1" pin="AGND" pad="58"/>
<connect gate="G$1" pin="AVDD" pad="59"/>
<connect gate="G$1" pin="DAC0/ADC12" pad="9"/>
<connect gate="G$1" pin="DAC1/ADC13" pad="10"/>
<connect gate="G$1" pin="DACGND" pad="57"/>
<connect gate="G$1" pin="DACREF" pad="56"/>
<connect gate="G$1" pin="DACVDD" pad="60"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="GNDREF" pad="7"/>
<connect gate="G$1" pin="IOGND" pad="19"/>
<connect gate="G$1" pin="IOGND@1" pad="41"/>
<connect gate="G$1" pin="IOVDD" pad="20"/>
<connect gate="G$1" pin="IOVDD@1" pad="42"/>
<connect gate="G$1" pin="LVDD" pad="21"/>
<connect gate="G$1" pin="P0.0/BM/CMPOUT/MS2" pad="15"/>
<connect gate="G$1" pin="P0.3/TRST/A16" pad="27"/>
<connect gate="G$1" pin="P0.4/IRQ0" pad="31"/>
<connect gate="G$1" pin="P0.5/IRQ1" pad="32"/>
<connect gate="G$1" pin="P0.6/T1/MRST/AE" pad="16"/>
<connect gate="G$1" pin="P0.7/ECLK/XCLK" pad="34"/>
<connect gate="G$1" pin="P1.0/T1/SPM0" pad="50"/>
<connect gate="G$1" pin="P1.1/SPM1" pad="49"/>
<connect gate="G$1" pin="P1.2/SPM2" pad="48"/>
<connect gate="G$1" pin="P1.3/SPM3" pad="47"/>
<connect gate="G$1" pin="P1.4/SPM4/IRQ2" pad="46"/>
<connect gate="G$1" pin="P1.5/SPM5/IRQ3" pad="45"/>
<connect gate="G$1" pin="P1.6/SPM6" pad="40"/>
<connect gate="G$1" pin="P1.7/SPM7" pad="39"/>
<connect gate="G$1" pin="P2.0/SPM9/!CONVSTART" pad="33"/>
<connect gate="G$1" pin="P3.0/AD0/PWM0H" pad="23"/>
<connect gate="G$1" pin="P3.1/AD1/PWM0L" pad="24"/>
<connect gate="G$1" pin="P3.2/AD2/PWM1H" pad="25"/>
<connect gate="G$1" pin="P3.3/AD3/PWM1L" pad="26"/>
<connect gate="G$1" pin="P3.4/AD4/PWM2H" pad="29"/>
<connect gate="G$1" pin="P3.5/AD5/PWM2L" pad="30"/>
<connect gate="G$1" pin="P3.6/AD6/PWMTRIP" pad="37"/>
<connect gate="G$1" pin="P3.7/AD7/PWMSYNC" pad="38"/>
<connect gate="G$1" pin="P4.0/AD8" pad="43"/>
<connect gate="G$1" pin="P4.1/AD9" pad="44"/>
<connect gate="G$1" pin="P4.2/AD10" pad="51"/>
<connect gate="G$1" pin="P4.3/AD11" pad="52"/>
<connect gate="G$1" pin="P4.4/AD12" pad="53"/>
<connect gate="G$1" pin="P4.5/AD13" pad="54"/>
<connect gate="G$1" pin="P4.6/AD14" pad="13"/>
<connect gate="G$1" pin="P4.7/AD15" pad="14"/>
<connect gate="G$1" pin="TCK" pad="17"/>
<connect gate="G$1" pin="TDI" pad="12"/>
<connect gate="G$1" pin="TDO" pad="18"/>
<connect gate="G$1" pin="TMS" pad="11"/>
<connect gate="G$1" pin="VREF" pad="55"/>
<connect gate="G$1" pin="XCLKI" pad="36"/>
<connect gate="G$1" pin="XCLKO" pad="35"/>
</connects>
<technologies>
<technology name="32">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="32-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="32-RL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="62">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="62-RL7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5BSTZ" package="LQFP-ST-64-2">
<connects>
<connect gate="G$1" pin="!RST" pad="28"/>
<connect gate="G$1" pin="ADC0" pad="61"/>
<connect gate="G$1" pin="ADC1" pad="62"/>
<connect gate="G$1" pin="ADC2/CMP0" pad="63"/>
<connect gate="G$1" pin="ADC3/CMP1" pad="64"/>
<connect gate="G$1" pin="ADC4" pad="1"/>
<connect gate="G$1" pin="ADC5" pad="2"/>
<connect gate="G$1" pin="ADC6" pad="3"/>
<connect gate="G$1" pin="ADC7" pad="4"/>
<connect gate="G$1" pin="ADC8" pad="5"/>
<connect gate="G$1" pin="ADC9" pad="6"/>
<connect gate="G$1" pin="ADCNEG" pad="8"/>
<connect gate="G$1" pin="AGND" pad="58"/>
<connect gate="G$1" pin="AVDD" pad="59"/>
<connect gate="G$1" pin="DAC0/ADC12" pad="9"/>
<connect gate="G$1" pin="DAC1/ADC13" pad="10"/>
<connect gate="G$1" pin="DACGND" pad="57"/>
<connect gate="G$1" pin="DACREF" pad="56"/>
<connect gate="G$1" pin="DACVDD" pad="60"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="GNDREF" pad="7"/>
<connect gate="G$1" pin="IOGND" pad="19"/>
<connect gate="G$1" pin="IOGND@1" pad="41"/>
<connect gate="G$1" pin="IOVDD" pad="20"/>
<connect gate="G$1" pin="IOVDD@1" pad="42"/>
<connect gate="G$1" pin="LVDD" pad="21"/>
<connect gate="G$1" pin="P0.0/BM/CMPOUT/MS2" pad="15"/>
<connect gate="G$1" pin="P0.3/TRST/A16" pad="27"/>
<connect gate="G$1" pin="P0.4/IRQ0" pad="31"/>
<connect gate="G$1" pin="P0.5/IRQ1" pad="32"/>
<connect gate="G$1" pin="P0.6/T1/MRST/AE" pad="16"/>
<connect gate="G$1" pin="P0.7/ECLK/XCLK" pad="34"/>
<connect gate="G$1" pin="P1.0/T1/SPM0" pad="50"/>
<connect gate="G$1" pin="P1.1/SPM1" pad="49"/>
<connect gate="G$1" pin="P1.2/SPM2" pad="48"/>
<connect gate="G$1" pin="P1.3/SPM3" pad="47"/>
<connect gate="G$1" pin="P1.4/SPM4/IRQ2" pad="46"/>
<connect gate="G$1" pin="P1.5/SPM5/IRQ3" pad="45"/>
<connect gate="G$1" pin="P1.6/SPM6" pad="40"/>
<connect gate="G$1" pin="P1.7/SPM7" pad="39"/>
<connect gate="G$1" pin="P2.0/SPM9/!CONVSTART" pad="33"/>
<connect gate="G$1" pin="P3.0/AD0/PWM0H" pad="23"/>
<connect gate="G$1" pin="P3.1/AD1/PWM0L" pad="24"/>
<connect gate="G$1" pin="P3.2/AD2/PWM1H" pad="25"/>
<connect gate="G$1" pin="P3.3/AD3/PWM1L" pad="26"/>
<connect gate="G$1" pin="P3.4/AD4/PWM2H" pad="29"/>
<connect gate="G$1" pin="P3.5/AD5/PWM2L" pad="30"/>
<connect gate="G$1" pin="P3.6/AD6/PWMTRIP" pad="37"/>
<connect gate="G$1" pin="P3.7/AD7/PWMSYNC" pad="38"/>
<connect gate="G$1" pin="P4.0/AD8" pad="43"/>
<connect gate="G$1" pin="P4.1/AD9" pad="44"/>
<connect gate="G$1" pin="P4.2/AD10" pad="51"/>
<connect gate="G$1" pin="P4.3/AD11" pad="52"/>
<connect gate="G$1" pin="P4.4/AD12" pad="53"/>
<connect gate="G$1" pin="P4.5/AD13" pad="54"/>
<connect gate="G$1" pin="P4.6/AD14" pad="13"/>
<connect gate="G$1" pin="P4.7/AD15" pad="14"/>
<connect gate="G$1" pin="TCK" pad="17"/>
<connect gate="G$1" pin="TDI" pad="12"/>
<connect gate="G$1" pin="TDO" pad="18"/>
<connect gate="G$1" pin="TMS" pad="11"/>
<connect gate="G$1" pin="VREF" pad="55"/>
<connect gate="G$1" pin="XCLKI" pad="36"/>
<connect gate="G$1" pin="XCLKO" pad="35"/>
</connects>
<technologies>
<technology name="62">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7025BSTZ62-RL"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8345"/>
</technology>
<technology name="62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC7*" prefix="IC">
<description>&lt;b&gt;Precision Analog Microcontroller 12-bit Analog I/O, ARM7TDMI® MCU&lt;/b&gt;&lt;p&gt;
ADuC7026/27&lt;br&gt;
Source: Source: http://www.analog.com/UploadedFiles/Data_Sheets/288945048AD7C7019_20_1_2_4_5_6_7_0.pdf</description>
<gates>
<gate name="G$1" symbol="ADUC70XX"/>
</gates>
<devices>
<device name="" package="LQFP_ST-80-1">
<connects>
<connect gate="G$1" pin="!RST" pad="37"/>
<connect gate="G$1" pin="ADC0" pad="77"/>
<connect gate="G$1" pin="ADC1" pad="78"/>
<connect gate="G$1" pin="ADC10" pad="7"/>
<connect gate="G$1" pin="ADC11" pad="76"/>
<connect gate="G$1" pin="ADC2/CMP0" pad="79"/>
<connect gate="G$1" pin="ADC3/CMP1" pad="80"/>
<connect gate="G$1" pin="ADC4" pad="1"/>
<connect gate="G$1" pin="ADC5" pad="2"/>
<connect gate="G$1" pin="ADC6" pad="3"/>
<connect gate="G$1" pin="ADC7" pad="4"/>
<connect gate="G$1" pin="ADC8" pad="5"/>
<connect gate="G$1" pin="ADC9" pad="6"/>
<connect gate="G$1" pin="ADCNEG" pad="9"/>
<connect gate="G$1" pin="AGND" pad="71"/>
<connect gate="G$1" pin="AGND@1" pad="72"/>
<connect gate="G$1" pin="AVDD" pad="73"/>
<connect gate="G$1" pin="AVDD@1" pad="74"/>
<connect gate="G$1" pin="DAC0/ADC12" pad="10"/>
<connect gate="G$1" pin="DAC1/ADC13" pad="11"/>
<connect gate="G$1" pin="DAC2/ADC14" pad="12"/>
<connect gate="G$1" pin="DAC3/ADC15" pad="13"/>
<connect gate="G$1" pin="DACGND" pad="70"/>
<connect gate="G$1" pin="DACREF" pad="69"/>
<connect gate="G$1" pin="DACVDD" pad="75"/>
<connect gate="G$1" pin="DGND" pad="28"/>
<connect gate="G$1" pin="GNDREF" pad="8"/>
<connect gate="G$1" pin="IOGND" pad="25"/>
<connect gate="G$1" pin="IOGND@1" pad="53"/>
<connect gate="G$1" pin="IOVDD" pad="26"/>
<connect gate="G$1" pin="IOVDD@1" pad="54"/>
<connect gate="G$1" pin="LVDD" pad="27"/>
<connect gate="G$1" pin="P0.0/BM/CMPOUT/MS2" pad="20"/>
<connect gate="G$1" pin="P0.1/!BLE" pad="16"/>
<connect gate="G$1" pin="P0.2/!BHE" pad="24"/>
<connect gate="G$1" pin="P0.3/TRST/A16" pad="34"/>
<connect gate="G$1" pin="P0.4/IRQ0" pad="40"/>
<connect gate="G$1" pin="P0.5/IRQ1" pad="41"/>
<connect gate="G$1" pin="P0.6/T1/MRST/AE" pad="21"/>
<connect gate="G$1" pin="P0.7/ECLK/XCLK" pad="43"/>
<connect gate="G$1" pin="P1.0/T1/SPM0" pad="62"/>
<connect gate="G$1" pin="P1.1/SPM1" pad="61"/>
<connect gate="G$1" pin="P1.2/SPM2" pad="60"/>
<connect gate="G$1" pin="P1.3/SPM3" pad="59"/>
<connect gate="G$1" pin="P1.4/SPM4/IRQ2" pad="58"/>
<connect gate="G$1" pin="P1.5/SPM5/IRQ3" pad="57"/>
<connect gate="G$1" pin="P1.6/SPM6" pad="52"/>
<connect gate="G$1" pin="P1.7/SPM7" pad="51"/>
<connect gate="G$1" pin="P2.0/SPM9/!CONVSTART" pad="42"/>
<connect gate="G$1" pin="P2.1/!WS" pad="49"/>
<connect gate="G$1" pin="P2.2/!RS" pad="50"/>
<connect gate="G$1" pin="P2.3/AE" pad="17"/>
<connect gate="G$1" pin="P2.4/MS0" pad="33"/>
<connect gate="G$1" pin="P2.5/MS1" pad="35"/>
<connect gate="G$1" pin="P2.6/MS2" pad="36"/>
<connect gate="G$1" pin="P2.7/MS3" pad="48"/>
<connect gate="G$1" pin="P3.0/AD0/PWM0H" pad="29"/>
<connect gate="G$1" pin="P3.1/AD1/PWM0L" pad="30"/>
<connect gate="G$1" pin="P3.2/AD2/PWM1H" pad="31"/>
<connect gate="G$1" pin="P3.3/AD3/PWM1L" pad="32"/>
<connect gate="G$1" pin="P3.4/AD4/PWM2H" pad="38"/>
<connect gate="G$1" pin="P3.5/AD5/PWM2L" pad="39"/>
<connect gate="G$1" pin="P3.6/AD6/PWMTRIP" pad="46"/>
<connect gate="G$1" pin="P3.7/AD7/PWMSYNC" pad="47"/>
<connect gate="G$1" pin="P4.0/AD8" pad="55"/>
<connect gate="G$1" pin="P4.1/AD9" pad="56"/>
<connect gate="G$1" pin="P4.2/AD10" pad="63"/>
<connect gate="G$1" pin="P4.3/AD11" pad="64"/>
<connect gate="G$1" pin="P4.4/AD12" pad="65"/>
<connect gate="G$1" pin="P4.5/AD13" pad="66"/>
<connect gate="G$1" pin="P4.6/AD14" pad="18"/>
<connect gate="G$1" pin="P4.7/AD15" pad="19"/>
<connect gate="G$1" pin="REFGND" pad="67"/>
<connect gate="G$1" pin="TCK" pad="22"/>
<connect gate="G$1" pin="TDI" pad="15"/>
<connect gate="G$1" pin="TDO" pad="23"/>
<connect gate="G$1" pin="TMS" pad="14"/>
<connect gate="G$1" pin="VREF" pad="68"/>
<connect gate="G$1" pin="XCLKI" pad="45"/>
<connect gate="G$1" pin="XCLKO" pad="44"/>
</connects>
<technologies>
<technology name="026BSTZ62">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7026BSTZ62"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8346"/>
</technology>
<technology name="026BSTZ62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="026BSTZ62I">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7026BSTZ62I-RL"/>
<attribute name="OC_FARNELL" value="1162647"/>
<attribute name="OC_NEWARK" value="12M8348"/>
</technology>
<technology name="026BSTZ62I-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="027BSTZ62">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7027BSTZ62"/>
<attribute name="OC_FARNELL" value="1162648"/>
<attribute name="OC_NEWARK" value="19M0746"/>
</technology>
<technology name="027BSTZ62-RL">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC7027BSTZ62-RL"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8350"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8612" prefix="IC">
<description>&lt;b&gt;Ultrafast 4 ns Single Supply Comparators&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf&lt;br&gt;
Upgrade for LT1394 and LT1016 Designs</description>
<gates>
<gate name="B" symbol="AD8612"/>
<gate name="A" symbol="AD8611"/>
</gates>
<devices>
<device name="RU" package="TSSOP14">
<connects>
<connect gate="A" pin="!OUT" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN+" pad="7"/>
<connect gate="A" pin="IN-" pad="6"/>
<connect gate="A" pin="L" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="5"/>
<connect gate="B" pin="!OUT" pad="13"/>
<connect gate="B" pin="GND" pad="12"/>
<connect gate="B" pin="IN+" pad="8"/>
<connect gate="B" pin="IN-" pad="9"/>
<connect gate="B" pin="L" pad="11"/>
<connect gate="B" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8612ARUZ"/>
<attribute name="OC_FARNELL" value="1464996"/>
<attribute name="OC_NEWARK" value="88H0301"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8611" prefix="IC">
<description>&lt;b&gt;Ultrafast 4 ns Single Supply Comparators&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf&lt;br&gt;
Upgrade for LT1394 and LT1016 Designs</description>
<gates>
<gate name="G$1" symbol="AD8611"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="!OUT" pad="8"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN+" pad="2"/>
<connect gate="G$1" pin="IN-" pad="3"/>
<connect gate="G$1" pin="L" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8611ARMZ-R2"/>
<attribute name="OC_FARNELL" value="1319472"/>
<attribute name="OC_NEWARK" value="19M8930"/>
</technology>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="G$1" pin="!OUT" pad="8"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN+" pad="2"/>
<connect gate="G$1" pin="IN-" pad="3"/>
<connect gate="G$1" pin="L" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8611ARMZ-R2"/>
<attribute name="OC_FARNELL" value="1464995"/>
<attribute name="OC_NEWARK" value="19M8930"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8367" prefix="IC">
<description>&lt;b&gt;500 MHz, Linear-in-dB VGA with AGC Detector&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/477808511AD8367_a.pdf</description>
<gates>
<gate name="G$1" symbol="AD8367"/>
</gates>
<devices>
<device name="RU" package="TSSOP14">
<connects>
<connect gate="G$1" pin="DECL" pad="9"/>
<connect gate="G$1" pin="DETO" pad="6"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GAIN" pad="5"/>
<connect gate="G$1" pin="HPFL" pad="13"/>
<connect gate="G$1" pin="ICOM@1" pad="1"/>
<connect gate="G$1" pin="ICOM@2" pad="7"/>
<connect gate="G$1" pin="ICOM@3" pad="14"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="MODE" pad="4"/>
<connect gate="G$1" pin="OCOM" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="10"/>
<connect gate="G$1" pin="VPSI" pad="12"/>
<connect gate="G$1" pin="VPSO" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8367ARUZ-RL7"/>
<attribute name="OC_FARNELL" value="1424121"/>
<attribute name="OC_NEWARK" value="59K6673"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7142*" prefix="IC">
<description>&lt;b&gt;Programmable Capacitance-to-Digital Converter with Environmental Compensation&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/762180021AD7142_42_1_prd.pdf</description>
<gates>
<gate name="G$1" symbol="AD7142"/>
</gates>
<devices>
<device name="" package="LFCSP32">
<connects>
<connect gate="G$1" pin="!CS!/ADD1" pad="24"/>
<connect gate="G$1" pin="!INT" pad="25"/>
<connect gate="G$1" pin="!SRC" pad="16"/>
<connect gate="G$1" pin="AGND" pad="14"/>
<connect gate="G$1" pin="AVCC" pad="13"/>
<connect gate="G$1" pin="CIN0" pad="30"/>
<connect gate="G$1" pin="CIN1" pad="31"/>
<connect gate="G$1" pin="CIN10" pad="8"/>
<connect gate="G$1" pin="CIN11" pad="9"/>
<connect gate="G$1" pin="CIN12" pad="10"/>
<connect gate="G$1" pin="CIN13" pad="11"/>
<connect gate="G$1" pin="CIN2" pad="32"/>
<connect gate="G$1" pin="CIN3" pad="1"/>
<connect gate="G$1" pin="CIN4" pad="2"/>
<connect gate="G$1" pin="CIN5" pad="3"/>
<connect gate="G$1" pin="CIN6" pad="4"/>
<connect gate="G$1" pin="CIN7" pad="5"/>
<connect gate="G$1" pin="CIN8" pad="6"/>
<connect gate="G$1" pin="CIN9" pad="7"/>
<connect gate="G$1" pin="CSHIELD" pad="12"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@D1" pad="18"/>
<connect gate="G$1" pin="GND@D2" pad="19"/>
<connect gate="G$1" pin="GPIO" pad="26"/>
<connect gate="G$1" pin="SCLK" pad="23"/>
<connect gate="G$1" pin="SDI/ADD0" pad="22"/>
<connect gate="G$1" pin="SDO/SDA" pad="21"/>
<connect gate="G$1" pin="SRC" pad="15"/>
<connect gate="G$1" pin="TEST" pad="27"/>
<connect gate="G$1" pin="VCC@D" pad="17"/>
<connect gate="G$1" pin="VDRIVE" pad="20"/>
<connect gate="G$1" pin="VREF+" pad="28"/>
<connect gate="G$1" pin="VREF-" pad="29"/>
</connects>
<technologies>
<technology name="-1ACPZ">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD7142ACPZ"/>
<attribute name="OC_FARNELL" value="1498724"/>
<attribute name="OC_NEWARK" value="15P0769"/>
</technology>
<technology name="ACPZ">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD7142ACPZ"/>
<attribute name="OC_FARNELL" value="1498724"/>
<attribute name="OC_NEWARK" value="15P0769"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7992" prefix="IC">
<description>&lt;b&gt;2-Channel, 12-Bit ADC with I2C-Compatible Interface&lt;/b&gt; 10-Lead MSOP&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/224965274AD7992_0.pdf</description>
<gates>
<gate name="G$1" symbol="AD7992"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="G$1" pin="!CONVST" pad="1"/>
<connect gate="G$1" pin="AGND" pad="2"/>
<connect gate="G$1" pin="AGND@1" pad="7"/>
<connect gate="G$1" pin="ALERT" pad="8"/>
<connect gate="G$1" pin="AS" pad="6"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="VIN1" pad="5"/>
<connect gate="G$1" pin="VIN2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD7992BRMZ-0"/>
<attribute name="OC_FARNELL" value="1078311"/>
<attribute name="OC_NEWARK" value="31M4422"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_BF561" prefix="IC">
<description>&lt;b&gt;ADSP_BF561&lt;/b&gt;&lt;p&gt;
finishd by 439390897ADSP_BF561_a.pdf at 2006.06.08&lt;br&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 13&lt;/i&gt;&lt;br&gt;
Source: 37918753ADSP_BF561_256_MBGA_rev0_3.bsdl</description>
<gates>
<gate name="G$1" symbol="ADSP_BF561_256_MBGA"/>
</gates>
<devices>
<device name="-MBGA265" package="MPBGA256">
<connects>
<connect gate="G$1" pin="ABE_B0" pad="E11"/>
<connect gate="G$1" pin="ABE_B1" pad="B13"/>
<connect gate="G$1" pin="ABE_B2" pad="A14"/>
<connect gate="G$1" pin="ABE_B3" pad="A15"/>
<connect gate="G$1" pin="ADDR10" pad="A6"/>
<connect gate="G$1" pin="ADDR11" pad="C6"/>
<connect gate="G$1" pin="ADDR12" pad="B5"/>
<connect gate="G$1" pin="ADDR13" pad="E6"/>
<connect gate="G$1" pin="ADDR14" pad="A5"/>
<connect gate="G$1" pin="ADDR15" pad="E5"/>
<connect gate="G$1" pin="ADDR16" pad="B4"/>
<connect gate="G$1" pin="ADDR17" pad="F6"/>
<connect gate="G$1" pin="ADDR18" pad="B3"/>
<connect gate="G$1" pin="ADDR19" pad="C4"/>
<connect gate="G$1" pin="ADDR2" pad="D13"/>
<connect gate="G$1" pin="ADDR20" pad="A3"/>
<connect gate="G$1" pin="ADDR21" pad="F5"/>
<connect gate="G$1" pin="ADDR22" pad="B2"/>
<connect gate="G$1" pin="ADDR23" pad="D4"/>
<connect gate="G$1" pin="ADDR24" pad="A2"/>
<connect gate="G$1" pin="ADDR25" pad="C3"/>
<connect gate="G$1" pin="ADDR3" pad="G11"/>
<connect gate="G$1" pin="ADDR4" pad="B15"/>
<connect gate="G$1" pin="ADDR5" pad="G10"/>
<connect gate="G$1" pin="ADDR6" pad="B14"/>
<connect gate="G$1" pin="ADDR7" pad="C14"/>
<connect gate="G$1" pin="ADDR8" pad="F11"/>
<connect gate="G$1" pin="ADDR9" pad="D7"/>
<connect gate="G$1" pin="AMS_B0" pad="C8"/>
<connect gate="G$1" pin="AMS_B1" pad="B7"/>
<connect gate="G$1" pin="AMS_B2" pad="E7"/>
<connect gate="G$1" pin="AMS_B3" pad="A7"/>
<connect gate="G$1" pin="AOE_B" pad="C7"/>
<connect gate="G$1" pin="ARDY" pad="D9"/>
<connect gate="G$1" pin="ARE_B" pad="B8"/>
<connect gate="G$1" pin="AWE_B" pad="A8"/>
<connect gate="G$1" pin="BGH_B" pad="C12"/>
<connect gate="G$1" pin="BG_B" pad="A13"/>
<connect gate="G$1" pin="BMODE0" pad="M10"/>
<connect gate="G$1" pin="BMODE1" pad="N10"/>
<connect gate="G$1" pin="BR_B" pad="B12"/>
<connect gate="G$1" pin="BY_PASS" pad="G4"/>
<connect gate="G$1" pin="CLKIN" pad="F1"/>
<connect gate="G$1" pin="DATA0" pad="B16"/>
<connect gate="G$1" pin="DATA1" pad="C15"/>
<connect gate="G$1" pin="DATA10" pad="F12"/>
<connect gate="G$1" pin="DATA11" pad="F16"/>
<connect gate="G$1" pin="DATA12" pad="F14"/>
<connect gate="G$1" pin="DATA13" pad="G15"/>
<connect gate="G$1" pin="DATA14" pad="G13"/>
<connect gate="G$1" pin="DATA15" pad="G12"/>
<connect gate="G$1" pin="DATA16" pad="H12"/>
<connect gate="G$1" pin="DATA17" pad="H15"/>
<connect gate="G$1" pin="DATA18" pad="H13"/>
<connect gate="G$1" pin="DATA19" pad="H16"/>
<connect gate="G$1" pin="DATA2" pad="E12"/>
<connect gate="G$1" pin="DATA20" pad="H14"/>
<connect gate="G$1" pin="DATA21" pad="J15"/>
<connect gate="G$1" pin="DATA22" pad="J13"/>
<connect gate="G$1" pin="DATA23" pad="J16"/>
<connect gate="G$1" pin="DATA24" pad="K14"/>
<connect gate="G$1" pin="DATA25" pad="K15"/>
<connect gate="G$1" pin="DATA26" pad="K13"/>
<connect gate="G$1" pin="DATA27" pad="L15"/>
<connect gate="G$1" pin="DATA28" pad="K12"/>
<connect gate="G$1" pin="DATA29" pad="L16"/>
<connect gate="G$1" pin="DATA3" pad="C16"/>
<connect gate="G$1" pin="DATA30" pad="J12"/>
<connect gate="G$1" pin="DATA31" pad="M15"/>
<connect gate="G$1" pin="DATA4" pad="E14"/>
<connect gate="G$1" pin="DATA5" pad="D15"/>
<connect gate="G$1" pin="DATA6" pad="D16"/>
<connect gate="G$1" pin="DATA7" pad="E15"/>
<connect gate="G$1" pin="DATA8" pad="F13"/>
<connect gate="G$1" pin="DATA9" pad="F15"/>
<connect gate="G$1" pin="DR0PRI" pad="L12"/>
<connect gate="G$1" pin="DR0SEC" pad="P16"/>
<connect gate="G$1" pin="DR1PRI" pad="M12"/>
<connect gate="G$1" pin="DR1SEC" pad="T14"/>
<connect gate="G$1" pin="DT0PRI" pad="M16"/>
<connect gate="G$1" pin="DT0SEC" pad="N15"/>
<connect gate="G$1" pin="DT1PRI" pad="R15"/>
<connect gate="G$1" pin="DT1SEC" pad="T15"/>
<connect gate="G$1" pin="EMU_B" pad="R11"/>
<connect gate="G$1" pin="GND@1" pad="C5"/>
<connect gate="G$1" pin="GND@10" pad="J7"/>
<connect gate="G$1" pin="GND@11" pad="J11"/>
<connect gate="G$1" pin="GND@12" pad="K9"/>
<connect gate="G$1" pin="GND@13" pad="K10"/>
<connect gate="G$1" pin="GND@14" pad="N12"/>
<connect gate="G$1" pin="GND@2" pad="G2"/>
<connect gate="G$1" pin="GND@3" pad="G7"/>
<connect gate="G$1" pin="GND@4" pad="G8"/>
<connect gate="G$1" pin="GND@5" pad="H1"/>
<connect gate="G$1" pin="GND@6" pad="H2"/>
<connect gate="G$1" pin="GND@7" pad="H8"/>
<connect gate="G$1" pin="GND@8" pad="H9"/>
<connect gate="G$1" pin="GND@9" pad="H10"/>
<connect gate="G$1" pin="GND_EXT@0" pad="M4"/>
<connect gate="G$1" pin="GND_EXT@1" pad="L3"/>
<connect gate="G$1" pin="GND_EXT@10" pad="E13"/>
<connect gate="G$1" pin="GND_EXT@11" pad="G14"/>
<connect gate="G$1" pin="GND_EXT@12" pad="J14"/>
<connect gate="G$1" pin="GND_EXT@13" pad="L14"/>
<connect gate="G$1" pin="GND_EXT@14" pad="N14"/>
<connect gate="G$1" pin="GND_EXT@15" pad="P12"/>
<connect gate="G$1" pin="GND_EXT@16" pad="P9"/>
<connect gate="G$1" pin="GND_EXT@17" pad="P5"/>
<connect gate="G$1" pin="GND_EXT@18" pad="P2"/>
<connect gate="G$1" pin="GND_EXT@2" pad="E1"/>
<connect gate="G$1" pin="GND_EXT@3" pad="N7"/>
<connect gate="G$1" pin="GND_EXT@4" pad="D5"/>
<connect gate="G$1" pin="GND_EXT@5" pad="D6"/>
<connect gate="G$1" pin="GND_EXT@6" pad="D8"/>
<connect gate="G$1" pin="GND_EXT@7" pad="C11"/>
<connect gate="G$1" pin="GND_EXT@8" pad="C13"/>
<connect gate="G$1" pin="GND_EXT@9" pad="D14"/>
<connect gate="G$1" pin="GND_INT@0" pad="G6"/>
<connect gate="G$1" pin="GND_INT@1" pad="F8"/>
<connect gate="G$1" pin="GND_INT@2" pad="F10"/>
<connect gate="G$1" pin="GND_INT@3" pad="L11"/>
<connect gate="G$1" pin="GND_INT@4" pad="L9"/>
<connect gate="G$1" pin="GND_INT@5" pad="L7"/>
<connect gate="G$1" pin="GND_INT@6" pad="K7"/>
<connect gate="G$1" pin="MISO" pad="R12"/>
<connect gate="G$1" pin="MOSI" pad="N11"/>
<connect gate="G$1" pin="NMI_0" pad="P11"/>
<connect gate="G$1" pin="NMI_1" pad="R9"/>
<connect gate="G$1" pin="PF0" pad="P4"/>
<connect gate="G$1" pin="PF1" pad="N5"/>
<connect gate="G$1" pin="PF10" pad="R7"/>
<connect gate="G$1" pin="PF11" pad="P7"/>
<connect gate="G$1" pin="PF12" pad="T7"/>
<connect gate="G$1" pin="PF13" pad="N8"/>
<connect gate="G$1" pin="PF14" pad="R8"/>
<connect gate="G$1" pin="PF15" pad="P8"/>
<connect gate="G$1" pin="PF2" pad="T4"/>
<connect gate="G$1" pin="PF3" pad="M6"/>
<connect gate="G$1" pin="PF4" pad="R5"/>
<connect gate="G$1" pin="PF5" pad="P6"/>
<connect gate="G$1" pin="PF6" pad="T5"/>
<connect gate="G$1" pin="PF7" pad="M7"/>
<connect gate="G$1" pin="PF8" pad="R6"/>
<connect gate="G$1" pin="PF9" pad="N6"/>
<connect gate="G$1" pin="PPI1_CLK" pad="C2"/>
<connect gate="G$1" pin="PPI1_DATA0" pad="L1"/>
<connect gate="G$1" pin="PPI1_DATA1" pad="J5"/>
<connect gate="G$1" pin="PPI1_DATA10" pad="F4"/>
<connect gate="G$1" pin="PPI1_DATA11" pad="E2"/>
<connect gate="G$1" pin="PPI1_DATA12" pad="E3"/>
<connect gate="G$1" pin="PPI1_DATA13" pad="D1"/>
<connect gate="G$1" pin="PPI1_DATA14" pad="G5"/>
<connect gate="G$1" pin="PPI1_DATA15" pad="D2"/>
<connect gate="G$1" pin="PPI1_DATA2" pad="J3"/>
<connect gate="G$1" pin="PPI1_DATA3" pad="J4"/>
<connect gate="G$1" pin="PPI1_DATA4" pad="K2"/>
<connect gate="G$1" pin="PPI1_DATA5" pad="H5"/>
<connect gate="G$1" pin="PPI1_DATA6" pad="K1"/>
<connect gate="G$1" pin="PPI1_DATA7" pad="H4"/>
<connect gate="G$1" pin="PPI1_DATA8" pad="K3"/>
<connect gate="G$1" pin="PPI1_DATA9" pad="H3"/>
<connect gate="G$1" pin="PPI1_SYNC1" pad="E4"/>
<connect gate="G$1" pin="PPI1_SYNC2" pad="C1"/>
<connect gate="G$1" pin="PPI1_SYNC3" pad="D3"/>
<connect gate="G$1" pin="PPI2_CLK" pad="B1"/>
<connect gate="G$1" pin="PPI2_DATA0" pad="R4"/>
<connect gate="G$1" pin="PPI2_DATA1" pad="N4"/>
<connect gate="G$1" pin="PPI2_DATA10" pad="N2"/>
<connect gate="G$1" pin="PPI2_DATA11" pad="L6"/>
<connect gate="G$1" pin="PPI2_DATA12" pad="N1"/>
<connect gate="G$1" pin="PPI2_DATA13" pad="M2"/>
<connect gate="G$1" pin="PPI2_DATA14" pad="K5"/>
<connect gate="G$1" pin="PPI2_DATA15" pad="M1"/>
<connect gate="G$1" pin="PPI2_DATA2" pad="R3"/>
<connect gate="G$1" pin="PPI2_DATA3" pad="N3"/>
<connect gate="G$1" pin="PPI2_DATA4" pad="T2"/>
<connect gate="G$1" pin="PPI2_DATA5" pad="P3"/>
<connect gate="G$1" pin="PPI2_DATA6" pad="R2"/>
<connect gate="G$1" pin="PPI2_DATA7" pad="R1"/>
<connect gate="G$1" pin="PPI2_DATA8" pad="P1"/>
<connect gate="G$1" pin="PPI2_DATA9" pad="M3"/>
<connect gate="G$1" pin="PPI2_SYNC1" pad="K4"/>
<connect gate="G$1" pin="PPI2_SYNC2" pad="L2"/>
<connect gate="G$1" pin="PPI2_SYNC3" pad="L4"/>
<connect gate="G$1" pin="PSMON_GND" pad="M5"/>
<connect gate="G$1" pin="PSMON_VDD" pad="M13"/>
<connect gate="G$1" pin="RESET_B" pad="F3"/>
<connect gate="G$1" pin="RFS0" pad="R16"/>
<connect gate="G$1" pin="RFS1" pad="N13"/>
<connect gate="G$1" pin="RSCLK0" pad="P15"/>
<connect gate="G$1" pin="RSCLK1" pad="P13"/>
<connect gate="G$1" pin="RX" pad="T13"/>
<connect gate="G$1" pin="SA10" pad="D11"/>
<connect gate="G$1" pin="SCAS_B" pad="D10"/>
<connect gate="G$1" pin="SCK" pad="M11"/>
<connect gate="G$1" pin="SCKE" pad="B10"/>
<connect gate="G$1" pin="SCLK0" pad="A11"/>
<connect gate="G$1" pin="SCLK1" pad="A12"/>
<connect gate="G$1" pin="SLEEP" pad="T11"/>
<connect gate="G$1" pin="SMS_B0" pad="E9"/>
<connect gate="G$1" pin="SMS_B1" pad="B9"/>
<connect gate="G$1" pin="SMS_B2" pad="C9"/>
<connect gate="G$1" pin="SMS_B3" pad="A10"/>
<connect gate="G$1" pin="SRAS_B" pad="C10"/>
<connect gate="G$1" pin="SWE_B" pad="E10"/>
<connect gate="G$1" pin="TCK" pad="T9"/>
<connect gate="G$1" pin="TDI" pad="R10"/>
<connect gate="G$1" pin="TDO" pad="N9"/>
<connect gate="G$1" pin="TEST" pad="M9"/>
<connect gate="G$1" pin="TFS0" pad="L13"/>
<connect gate="G$1" pin="TFS1" pad="P14"/>
<connect gate="G$1" pin="TMS" pad="T10"/>
<connect gate="G$1" pin="TRST_B" pad="P10"/>
<connect gate="G$1" pin="TSCLK0" pad="N16"/>
<connect gate="G$1" pin="TSCLK1" pad="R14"/>
<connect gate="G$1" pin="TX" pad="R13"/>
<connect gate="G$1" pin="VDD_EXT@0" pad="T1"/>
<connect gate="G$1" pin="VDD_EXT@1" pad="L5"/>
<connect gate="G$1" pin="VDD_EXT@10" pad="E16"/>
<connect gate="G$1" pin="VDD_EXT@11" pad="G16"/>
<connect gate="G$1" pin="VDD_EXT@12" pad="K16"/>
<connect gate="G$1" pin="VDD_EXT@13" pad="M14"/>
<connect gate="G$1" pin="VDD_EXT@14" pad="T16"/>
<connect gate="G$1" pin="VDD_EXT@15" pad="T12"/>
<connect gate="G$1" pin="VDD_EXT@16" pad="T8"/>
<connect gate="G$1" pin="VDD_EXT@17" pad="T6"/>
<connect gate="G$1" pin="VDD_EXT@18" pad="T3"/>
<connect gate="G$1" pin="VDD_EXT@19" pad="G3"/>
<connect gate="G$1" pin="VDD_EXT@2" pad="F2"/>
<connect gate="G$1" pin="VDD_EXT@20" pad="J6"/>
<connect gate="G$1" pin="VDD_EXT@21" pad="K6"/>
<connect gate="G$1" pin="VDD_EXT@22" pad="L10"/>
<connect gate="G$1" pin="VDD_EXT@3" pad="A1"/>
<connect gate="G$1" pin="VDD_EXT@4" pad="A4"/>
<connect gate="G$1" pin="VDD_EXT@5" pad="B6"/>
<connect gate="G$1" pin="VDD_EXT@6" pad="A9"/>
<connect gate="G$1" pin="VDD_EXT@7" pad="B11"/>
<connect gate="G$1" pin="VDD_EXT@8" pad="D12"/>
<connect gate="G$1" pin="VDD_EXT@9" pad="A16"/>
<connect gate="G$1" pin="VDD_INT@0" pad="H7"/>
<connect gate="G$1" pin="VDD_INT@1" pad="F7"/>
<connect gate="G$1" pin="VDD_INT@10" pad="H6"/>
<connect gate="G$1" pin="VDD_INT@11" pad="K11"/>
<connect gate="G$1" pin="VDD_INT@12" pad="L8"/>
<connect gate="G$1" pin="VDD_INT@13" pad="M8"/>
<connect gate="G$1" pin="VDD_INT@2" pad="E8"/>
<connect gate="G$1" pin="VDD_INT@3" pad="G9"/>
<connect gate="G$1" pin="VDD_INT@4" pad="H11"/>
<connect gate="G$1" pin="VDD_INT@5" pad="J10"/>
<connect gate="G$1" pin="VDD_INT@6" pad="J9"/>
<connect gate="G$1" pin="VDD_INT@7" pad="K8"/>
<connect gate="G$1" pin="VDD_INT@8" pad="J8"/>
<connect gate="G$1" pin="VDD_INT@9" pad="F9"/>
<connect gate="G$1" pin="VREF_FLT" pad="J2"/>
<connect gate="G$1" pin="VREG" pad="J1"/>
<connect gate="G$1" pin="XTAL" pad="G1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8067" prefix="IC">
<description>&lt;b&gt;High Gain Bandwidth, Precision Fast FET&lt;/b&gt;(TM)&lt;b&gt; Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/346131962AD8067_a.pdf</description>
<gates>
<gate name="G$1" symbol="OP+-VS"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+VS" pad="5"/>
<connect gate="G$1" pin="-VS" pad="2"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8067ARTZ-REEL7"/>
<attribute name="OC_FARNELL" value="1464848"/>
<attribute name="OC_NEWARK" value="59K6326"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7714" prefix="IC">
<description>&lt;b&gt;Signal Conditioning ADC&lt;/b&gt; 3 V/5 V, CMOS, 500 mA&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/39677768AD7714_c.pdf</description>
<gates>
<gate name="G$1" symbol="AD7714"/>
</gates>
<devices>
<device name="R-24" package="SO24R">
<connects>
<connect gate="G$1" pin="!CS" pad="19"/>
<connect gate="G$1" pin="!DRDY" pad="20"/>
<connect gate="G$1" pin="!RESET" pad="6"/>
<connect gate="G$1" pin="!STANDBY" pad="11"/>
<connect gate="G$1" pin="!SYNC" pad="5"/>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="AIN1" pad="7"/>
<connect gate="G$1" pin="AIN2" pad="8"/>
<connect gate="G$1" pin="AIN3" pad="9"/>
<connect gate="G$1" pin="AIN4" pad="10"/>
<connect gate="G$1" pin="AIN5" pad="16"/>
<connect gate="G$1" pin="AIN6" pad="17"/>
<connect gate="G$1" pin="AVDD" pad="12"/>
<connect gate="G$1" pin="BUFFER" pad="13"/>
<connect gate="G$1" pin="DGND" pad="24"/>
<connect gate="G$1" pin="DIN" pad="22"/>
<connect gate="G$1" pin="DOUT" pad="21"/>
<connect gate="G$1" pin="DVDD" pad="23"/>
<connect gate="G$1" pin="MCLKIN" pad="2"/>
<connect gate="G$1" pin="MCLKOUT" pad="3"/>
<connect gate="G$1" pin="POL" pad="4"/>
<connect gate="G$1" pin="REFIN+" pad="15"/>
<connect gate="G$1" pin="REFIN-" pad="14"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="RS-28" package="SSOP28">
<connects>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="!DRDY" pad="24"/>
<connect gate="G$1" pin="!RESET" pad="6"/>
<connect gate="G$1" pin="!STANDBY" pad="13"/>
<connect gate="G$1" pin="!SYNC" pad="5"/>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AIN1" pad="9"/>
<connect gate="G$1" pin="AIN2" pad="10"/>
<connect gate="G$1" pin="AIN3" pad="11"/>
<connect gate="G$1" pin="AIN4" pad="12"/>
<connect gate="G$1" pin="AIN5" pad="18"/>
<connect gate="G$1" pin="AIN6" pad="19"/>
<connect gate="G$1" pin="AVDD" pad="14"/>
<connect gate="G$1" pin="BUFFER" pad="15"/>
<connect gate="G$1" pin="DGND" pad="28"/>
<connect gate="G$1" pin="DIN" pad="26"/>
<connect gate="G$1" pin="DOUT" pad="25"/>
<connect gate="G$1" pin="DVDD" pad="27"/>
<connect gate="G$1" pin="MCLKIN" pad="2"/>
<connect gate="G$1" pin="MCLKOUT" pad="3"/>
<connect gate="G$1" pin="POL" pad="4"/>
<connect gate="G$1" pin="REFIN+" pad="17"/>
<connect gate="G$1" pin="REFIN-" pad="16"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7714ARS-3"/>
<attribute name="OC_FARNELL" value="1423921"/>
<attribute name="OC_NEWARK" value="52F2117"/>
</technology>
</technologies>
</device>
<device name="RU-24" package="TSSOP24">
<connects>
<connect gate="G$1" pin="!CS" pad="19"/>
<connect gate="G$1" pin="!DRDY" pad="20"/>
<connect gate="G$1" pin="!RESET" pad="6"/>
<connect gate="G$1" pin="!STANDBY" pad="11"/>
<connect gate="G$1" pin="!SYNC" pad="5"/>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="AIN1" pad="7"/>
<connect gate="G$1" pin="AIN2" pad="8"/>
<connect gate="G$1" pin="AIN3" pad="9"/>
<connect gate="G$1" pin="AIN4" pad="10"/>
<connect gate="G$1" pin="AIN5" pad="16"/>
<connect gate="G$1" pin="AIN6" pad="17"/>
<connect gate="G$1" pin="AVDD" pad="12"/>
<connect gate="G$1" pin="BUFFER" pad="13"/>
<connect gate="G$1" pin="DGND" pad="24"/>
<connect gate="G$1" pin="DIN" pad="22"/>
<connect gate="G$1" pin="DOUT" pad="21"/>
<connect gate="G$1" pin="DVDD" pad="23"/>
<connect gate="G$1" pin="MCLKIN" pad="2"/>
<connect gate="G$1" pin="MCLKOUT" pad="3"/>
<connect gate="G$1" pin="POL" pad="4"/>
<connect gate="G$1" pin="REFIN+" pad="15"/>
<connect gate="G$1" pin="REFIN-" pad="14"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD7714YRUZ"/>
<attribute name="OC_FARNELL" value="1438857"/>
<attribute name="OC_NEWARK" value="19M8848"/>
</technology>
</technologies>
</device>
<device name="N-24" package="DIL24-3">
<connects>
<connect gate="G$1" pin="!CS" pad="19"/>
<connect gate="G$1" pin="!DRDY" pad="20"/>
<connect gate="G$1" pin="!RESET" pad="6"/>
<connect gate="G$1" pin="!STANDBY" pad="11"/>
<connect gate="G$1" pin="!SYNC" pad="5"/>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="AIN1" pad="7"/>
<connect gate="G$1" pin="AIN2" pad="8"/>
<connect gate="G$1" pin="AIN3" pad="9"/>
<connect gate="G$1" pin="AIN4" pad="10"/>
<connect gate="G$1" pin="AIN5" pad="16"/>
<connect gate="G$1" pin="AIN6" pad="17"/>
<connect gate="G$1" pin="AVDD" pad="12"/>
<connect gate="G$1" pin="BUFFER" pad="13"/>
<connect gate="G$1" pin="DGND" pad="24"/>
<connect gate="G$1" pin="DIN" pad="22"/>
<connect gate="G$1" pin="DOUT" pad="21"/>
<connect gate="G$1" pin="DVDD" pad="23"/>
<connect gate="G$1" pin="MCLKIN" pad="2"/>
<connect gate="G$1" pin="MCLKOUT" pad="3"/>
<connect gate="G$1" pin="POL" pad="4"/>
<connect gate="G$1" pin="REFIN+" pad="15"/>
<connect gate="G$1" pin="REFIN-" pad="14"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7714AN-5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="66F5871"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD421" prefix="IC">
<description>&lt;b&gt;Loop-Powered 4 mA to 20 mA DAC&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/409317160AD421_c.pdf</description>
<gates>
<gate name="G$1" symbol="AD421"/>
</gates>
<devices>
<device name="BN" package="DIL16">
<connects>
<connect gate="G$1" pin="BOOST" pad="15"/>
<connect gate="G$1" pin="C1" pad="12"/>
<connect gate="G$1" pin="C2" pad="11"/>
<connect gate="G$1" pin="C3" pad="10"/>
<connect gate="G$1" pin="CLOCK" pad="6"/>
<connect gate="G$1" pin="COM" pad="9"/>
<connect gate="G$1" pin="COMP" pad="14"/>
<connect gate="G$1" pin="DATA" pad="7"/>
<connect gate="G$1" pin="DRIVE" pad="13"/>
<connect gate="G$1" pin="LATCH" pad="5"/>
<connect gate="G$1" pin="LOOP-RTN" pad="8"/>
<connect gate="G$1" pin="LV" pad="4"/>
<connect gate="G$1" pin="REFIN" pad="3"/>
<connect gate="G$1" pin="REFOUT1" pad="1"/>
<connect gate="G$1" pin="REFOUT2" pad="2"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD421BN"/>
<attribute name="OC_FARNELL" value="1438368"/>
<attribute name="OC_NEWARK" value="52F8047"/>
</technology>
</technologies>
</device>
<device name="BR" package="SO-16W">
<connects>
<connect gate="G$1" pin="BOOST" pad="15"/>
<connect gate="G$1" pin="C1" pad="12"/>
<connect gate="G$1" pin="C2" pad="11"/>
<connect gate="G$1" pin="C3" pad="10"/>
<connect gate="G$1" pin="CLOCK" pad="6"/>
<connect gate="G$1" pin="COM" pad="9"/>
<connect gate="G$1" pin="COMP" pad="14"/>
<connect gate="G$1" pin="DATA" pad="7"/>
<connect gate="G$1" pin="DRIVE" pad="13"/>
<connect gate="G$1" pin="LATCH" pad="5"/>
<connect gate="G$1" pin="LOOP-RTN" pad="8"/>
<connect gate="G$1" pin="LV" pad="4"/>
<connect gate="G$1" pin="REFIN" pad="3"/>
<connect gate="G$1" pin="REFOUT1" pad="1"/>
<connect gate="G$1" pin="REFOUT2" pad="2"/>
<connect gate="G$1" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD421BR"/>
<attribute name="OC_FARNELL" value="1278822"/>
<attribute name="OC_NEWARK" value="52F8048"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9859" prefix="IC">
<description>&lt;b&gt;CMOS Direct Digital Synthesizer&lt;/b&gt; 400 MSPS, 10-Bit, 1.8 V&lt;p&gt;
Source: www.analog.com/UploadedFiles/Data_Sheets/33830397585263AD9859_0.pdf</description>
<gates>
<gate name="G$1" symbol="AD9859"/>
</gates>
<devices>
<device name="" package="QFP-7X7-48">
<connects>
<connect gate="G$1" pin="!CS" pad="39"/>
<connect gate="G$1" pin="!IOUT" pad="20"/>
<connect gate="G$1" pin="!OSC/!REFCLK" pad="8"/>
<connect gate="G$1" pin="AGND/EXP" pad="EXP"/>
<connect gate="G$1" pin="AGND@1" pad="5"/>
<connect gate="G$1" pin="AGND@10" pad="32"/>
<connect gate="G$1" pin="AGND@11" pad="31"/>
<connect gate="G$1" pin="AGND@2" pad="7"/>
<connect gate="G$1" pin="AGND@3" pad="14"/>
<connect gate="G$1" pin="AGND@4" pad="15"/>
<connect gate="G$1" pin="AGND@5" pad="17"/>
<connect gate="G$1" pin="AGND@6" pad="22"/>
<connect gate="G$1" pin="AGND@7" pad="26"/>
<connect gate="G$1" pin="AGND@8" pad="28"/>
<connect gate="G$1" pin="AGND@9" pad="30"/>
<connect gate="G$1" pin="AVDD@1" pad="4"/>
<connect gate="G$1" pin="AVDD@2" pad="6"/>
<connect gate="G$1" pin="AVDD@3" pad="13"/>
<connect gate="G$1" pin="AVDD@4" pad="16"/>
<connect gate="G$1" pin="AVDD@5" pad="18"/>
<connect gate="G$1" pin="AVDD@6" pad="19"/>
<connect gate="G$1" pin="AVDD@7" pad="25"/>
<connect gate="G$1" pin="AVDD@8" pad="27"/>
<connect gate="G$1" pin="AVDD@9" pad="29"/>
<connect gate="G$1" pin="CLKMODESELECT" pad="11"/>
<connect gate="G$1" pin="CRYSTAL_OUT" pad="10"/>
<connect gate="G$1" pin="DACBP" pad="23"/>
<connect gate="G$1" pin="DAC_RSET" pad="24"/>
<connect gate="G$1" pin="DGND@1" pad="3"/>
<connect gate="G$1" pin="DGND@2" pad="33"/>
<connect gate="G$1" pin="DGND@3" pad="42"/>
<connect gate="G$1" pin="DGND@4" pad="47"/>
<connect gate="G$1" pin="DGND@5" pad="48"/>
<connect gate="G$1" pin="DVDD@1" pad="2"/>
<connect gate="G$1" pin="DVDD@2" pad="34"/>
<connect gate="G$1" pin="DVDD_I/O" pad="43"/>
<connect gate="G$1" pin="I/O_UPDATE" pad="1"/>
<connect gate="G$1" pin="IOSYNC" pad="37"/>
<connect gate="G$1" pin="IOUT" pad="21"/>
<connect gate="G$1" pin="LOOP_FILTER" pad="12"/>
<connect gate="G$1" pin="OSC/REFCLK" pad="9"/>
<connect gate="G$1" pin="OSK" pad="46"/>
<connect gate="G$1" pin="PWRDWNCTL" pad="35"/>
<connect gate="G$1" pin="RESET" pad="36"/>
<connect gate="G$1" pin="SCLK" pad="40"/>
<connect gate="G$1" pin="SDIO" pad="41"/>
<connect gate="G$1" pin="SDO" pad="38"/>
<connect gate="G$1" pin="SYNC_CLK" pad="45"/>
<connect gate="G$1" pin="SYNC_IN" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD9859YSVZ"/>
<attribute name="OC_FARNELL" value="1438601"/>
<attribute name="OC_NEWARK" value="59K7492"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7651" prefix="IC">
<description>&lt;b&gt;16-Bit 100 kSPS PulSARTM Unipolar ADC&lt;/b&gt; with Reference&lt;p&gt;
Source: COMPLIANT TO JEDEC STANDARDS MO-220-VKKD-2</description>
<gates>
<gate name="A" symbol="AD7651"/>
</gates>
<devices>
<device name="ACP" package="LFCSP48">
<connects>
<connect gate="A" pin="!CNVST" pad="35"/>
<connect gate="A" pin="!CS" pad="32"/>
<connect gate="A" pin="!RD" pad="31"/>
<connect gate="A" pin="AGND" pad="1"/>
<connect gate="A" pin="AGND@1" pad="36"/>
<connect gate="A" pin="AGND@2" pad="41"/>
<connect gate="A" pin="AGND@3" pad="42"/>
<connect gate="A" pin="AGND@EXP" pad="EXP"/>
<connect gate="A" pin="AVDD" pad="2"/>
<connect gate="A" pin="AVDD@1" pad="44"/>
<connect gate="A" pin="BUSY" pad="29"/>
<connect gate="A" pin="BYTESWAP" pad="4"/>
<connect gate="A" pin="D0" pad="9"/>
<connect gate="A" pin="D1" pad="10"/>
<connect gate="A" pin="D10" pad="23"/>
<connect gate="A" pin="D11" pad="24"/>
<connect gate="A" pin="D12" pad="25"/>
<connect gate="A" pin="D13" pad="26"/>
<connect gate="A" pin="D14" pad="27"/>
<connect gate="A" pin="D15" pad="28"/>
<connect gate="A" pin="D2" pad="11"/>
<connect gate="A" pin="D3" pad="12"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="15"/>
<connect gate="A" pin="D7" pad="16"/>
<connect gate="A" pin="D8" pad="21"/>
<connect gate="A" pin="D9" pad="22"/>
<connect gate="A" pin="DGND" pad="20"/>
<connect gate="A" pin="DGND@1" pad="30"/>
<connect gate="A" pin="DVDD" pad="19"/>
<connect gate="A" pin="IN" pad="43"/>
<connect gate="A" pin="INGND" pad="39"/>
<connect gate="A" pin="OB/!2C" pad="5"/>
<connect gate="A" pin="OGND" pad="17"/>
<connect gate="A" pin="OVDD" pad="18"/>
<connect gate="A" pin="PD" pad="34"/>
<connect gate="A" pin="PDBUF" pad="48"/>
<connect gate="A" pin="PDREF" pad="47"/>
<connect gate="A" pin="REF" pad="37"/>
<connect gate="A" pin="REFBUFIN" pad="46"/>
<connect gate="A" pin="REFGND" pad="38"/>
<connect gate="A" pin="RESET" pad="33"/>
<connect gate="A" pin="SER/!PAR" pad="8"/>
<connect gate="A" pin="TEMP" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="AST" package="QFP-7X7-48">
<connects>
<connect gate="A" pin="!CNVST" pad="35"/>
<connect gate="A" pin="!CS" pad="32"/>
<connect gate="A" pin="!RD" pad="31"/>
<connect gate="A" pin="AGND" pad="1"/>
<connect gate="A" pin="AGND@1" pad="36"/>
<connect gate="A" pin="AGND@2" pad="41"/>
<connect gate="A" pin="AGND@3" pad="42"/>
<connect gate="A" pin="AGND@EXP" pad="EXP"/>
<connect gate="A" pin="AVDD" pad="2"/>
<connect gate="A" pin="AVDD@1" pad="44"/>
<connect gate="A" pin="BUSY" pad="29"/>
<connect gate="A" pin="BYTESWAP" pad="4"/>
<connect gate="A" pin="D0" pad="9"/>
<connect gate="A" pin="D1" pad="10"/>
<connect gate="A" pin="D10" pad="23"/>
<connect gate="A" pin="D11" pad="24"/>
<connect gate="A" pin="D12" pad="25"/>
<connect gate="A" pin="D13" pad="26"/>
<connect gate="A" pin="D14" pad="27"/>
<connect gate="A" pin="D15" pad="28"/>
<connect gate="A" pin="D2" pad="11"/>
<connect gate="A" pin="D3" pad="12"/>
<connect gate="A" pin="D4" pad="13"/>
<connect gate="A" pin="D5" pad="14"/>
<connect gate="A" pin="D6" pad="15"/>
<connect gate="A" pin="D7" pad="16"/>
<connect gate="A" pin="D8" pad="21"/>
<connect gate="A" pin="D9" pad="22"/>
<connect gate="A" pin="DGND" pad="20"/>
<connect gate="A" pin="DGND@1" pad="30"/>
<connect gate="A" pin="DVDD" pad="19"/>
<connect gate="A" pin="IN" pad="43"/>
<connect gate="A" pin="INGND" pad="39"/>
<connect gate="A" pin="OB/!2C" pad="5"/>
<connect gate="A" pin="OGND" pad="17"/>
<connect gate="A" pin="OVDD" pad="18"/>
<connect gate="A" pin="PD" pad="34"/>
<connect gate="A" pin="PDBUF" pad="48"/>
<connect gate="A" pin="PDREF" pad="47"/>
<connect gate="A" pin="REF" pad="37"/>
<connect gate="A" pin="REFBUFIN" pad="46"/>
<connect gate="A" pin="REFGND" pad="38"/>
<connect gate="A" pin="RESET" pad="33"/>
<connect gate="A" pin="SER/!PAR" pad="8"/>
<connect gate="A" pin="TEMP" pad="45"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD7651ASTZ"/>
<attribute name="OC_FARNELL" value="1581929"/>
<attribute name="OC_NEWARK" value="15P0825"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG419" prefix="IC">
<description>&lt;b&gt;LC²MOS Precision Mini-DIP Analog switch&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/ADG419.pdf</description>
<gates>
<gate name="G$1" symbol="ADG419"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="6"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="8"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VL" pad="5"/>
<connect gate="G$1" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG419BN"/>
<attribute name="OC_FARNELL" value="1438705"/>
<attribute name="OC_NEWARK" value="16F6524"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD620" prefix="IC">
<description>&lt;b&gt;Low Cost, Low Power, Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/37793330023930AD620_e.pdf</description>
<gates>
<gate name="G$1" symbol="AD620"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="+V" pad="7"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="1"/>
<connect gate="G$1" pin="RG@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD620AR"/>
<attribute name="OC_FARNELL" value="1464424"/>
<attribute name="OC_NEWARK" value="05F7109"/>
</technology>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="+V" pad="7"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="1"/>
<connect gate="G$1" pin="RG@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD620AN"/>
<attribute name="OC_FARNELL" value="1523782"/>
<attribute name="OC_NEWARK" value="05F7108"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8353" prefix="IC">
<description>&lt;b&gt;1 MHz to 2.7 GHz RF Gain Block&lt;/b&gt;&lt;p&gt;
Source: AD8353.pdf</description>
<gates>
<gate name="G$1" symbol="AD8353"/>
</gates>
<devices>
<device name="" package="LFCSP_VD08">
<connects>
<connect gate="G$1" pin="COM1@1" pad="1"/>
<connect gate="G$1" pin="COM1@2" pad="8"/>
<connect gate="G$1" pin="COM2@1" pad="4"/>
<connect gate="G$1" pin="COM2@2" pad="5"/>
<connect gate="G$1" pin="EXP@1" pad="EXP@1"/>
<connect gate="G$1" pin="EXP@2" pad="EXP@2"/>
<connect gate="G$1" pin="RFIN" pad="3"/>
<connect gate="G$1" pin="RFOUT" pad="7"/>
<connect gate="G$1" pin="VPOS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8353ACPZ-REEL7"/>
<attribute name="OC_FARNELL" value="1346356"/>
<attribute name="OC_NEWARK" value="59K6665"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD780" prefix="IC">
<description>&lt;b&gt;High Precision Reference&lt;/b&gt; 2.5V/3.0V&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/AD780.pdf</description>
<gates>
<gate name="G$1" symbol="AD780"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="O/P" pad="8"/>
<connect gate="G$1" pin="TEMP" pad="3"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD780ANZ"/>
<attribute name="OC_FARNELL" value="9605550"/>
<attribute name="OC_NEWARK" value="59K5478"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+VIN" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="O/P" pad="8"/>
<connect gate="G$1" pin="TEMP" pad="3"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="VOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD780BRZ-REEL"/>
<attribute name="OC_FARNELL" value="1464655"/>
<attribute name="OC_NEWARK" value="12M8938"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9901" prefix="IC">
<description>&lt;b&gt;Ultrahigh Speed Phase/Frequency Discrimainator&lt;/b&gt; Phase-Locked-Loop&lt;p&gt;
Source: 36342005AD9901_b.pdf</description>
<gates>
<gate name="G$1" symbol="AD9901"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="G$1" pin="!OUT" pad="10"/>
<connect gate="G$1" pin="+VS@1" pad="7"/>
<connect gate="G$1" pin="+VS@2" pad="11"/>
<connect gate="G$1" pin="BIAS" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="1"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="GND@3" pad="4"/>
<connect gate="G$1" pin="GND@4" pad="8"/>
<connect gate="G$1" pin="GND@5" pad="13"/>
<connect gate="G$1" pin="GND@6" pad="14"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REFIN" pad="12"/>
<connect gate="G$1" pin="RSET" pad="9"/>
<connect gate="G$1" pin="VCOIN" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD9901KQ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="05F7832"/>
</technology>
</technologies>
</device>
<device name="PL" package="PLCC20">
<connects>
<connect gate="G$1" pin="!OUT" pad="14"/>
<connect gate="G$1" pin="+VS@1" pad="10"/>
<connect gate="G$1" pin="+VS@2" pad="16"/>
<connect gate="G$1" pin="BIAS" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="GND@3" pad="5"/>
<connect gate="G$1" pin="GND@4" pad="12"/>
<connect gate="G$1" pin="GND@5" pad="19"/>
<connect gate="G$1" pin="GND@6" pad="20"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="REFIN" pad="18"/>
<connect gate="G$1" pin="RSET" pad="13"/>
<connect gate="G$1" pin="VCOIN" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD9901KP"/>
<attribute name="OC_FARNELL" value="1424271"/>
<attribute name="OC_NEWARK" value="83F3495"/>
</technology>
</technologies>
</device>
<device name="LC" package="LCC20">
<connects>
<connect gate="G$1" pin="!OUT" pad="14"/>
<connect gate="G$1" pin="+VS@1" pad="10"/>
<connect gate="G$1" pin="+VS@2" pad="16"/>
<connect gate="G$1" pin="BIAS" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="12"/>
<connect gate="G$1" pin="GND@5" pad="19"/>
<connect gate="G$1" pin="GND@6" pad="20"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="REFIN" pad="18"/>
<connect gate="G$1" pin="RSET" pad="13"/>
<connect gate="G$1" pin="VCOIN" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD9901KPZ"/>
<attribute name="OC_FARNELL" value="1676470"/>
<attribute name="OC_NEWARK" value="59K7524"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7303B" prefix="IC">
<description>&lt;b&gt;+2.7 V to +5.5 V, Serial Input, Dual Voltage Output 8-Bit DAC&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/AD7303.pdf</description>
<gates>
<gate name="G$1" symbol="AD7303"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="!SYNC" pad="7"/>
<connect gate="G$1" pin="DIN" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VOUTA" pad="1"/>
<connect gate="G$1" pin="VOUTB" pad="8"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD7303BRZ"/>
<attribute name="OC_FARNELL" value="1838896"/>
<attribute name="OC_NEWARK" value="19M8835"/>
</technology>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="G$1" pin="!SYNC" pad="7"/>
<connect gate="G$1" pin="DIN" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VOUTA" pad="1"/>
<connect gate="G$1" pin="VOUTB" pad="8"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7303BRMZ"/>
<attribute name="OC_FARNELL" value="1464525"/>
<attribute name="OC_NEWARK" value="59K4694"/>
</technology>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="!SYNC" pad="7"/>
<connect gate="G$1" pin="DIN" pad="6"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="SCLK" pad="5"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VOUTA" pad="1"/>
<connect gate="G$1" pin="VOUTB" pad="8"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD7303BNZ"/>
<attribute name="OC_FARNELL" value="1079413"/>
<attribute name="OC_NEWARK" value="19M0854"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9951" prefix="IC">
<description>&lt;b&gt;14-bit DAC Direct Digital Synthesizer&lt;/b&gt; 400 MSPS 14-Bit, 1.8 V CMOS&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD9951.pdf</description>
<gates>
<gate name="G$1" symbol="AD9951"/>
</gates>
<devices>
<device name="EP" package="QFP-7X7-48">
<connects>
<connect gate="G$1" pin="!CS" pad="39"/>
<connect gate="G$1" pin="!IOUT" pad="20"/>
<connect gate="G$1" pin="!REFCLK" pad="8"/>
<connect gate="G$1" pin="AGND@1" pad="5"/>
<connect gate="G$1" pin="AGND@10" pad="31"/>
<connect gate="G$1" pin="AGND@11" pad="32"/>
<connect gate="G$1" pin="AGND@2" pad="7"/>
<connect gate="G$1" pin="AGND@3" pad="14"/>
<connect gate="G$1" pin="AGND@4" pad="15"/>
<connect gate="G$1" pin="AGND@5" pad="17"/>
<connect gate="G$1" pin="AGND@6" pad="22"/>
<connect gate="G$1" pin="AGND@7" pad="26"/>
<connect gate="G$1" pin="AGND@8" pad="28"/>
<connect gate="G$1" pin="AGND@9" pad="30"/>
<connect gate="G$1" pin="AVDD@1" pad="4"/>
<connect gate="G$1" pin="AVDD@2" pad="6"/>
<connect gate="G$1" pin="AVDD@3" pad="13"/>
<connect gate="G$1" pin="AVDD@4" pad="16"/>
<connect gate="G$1" pin="AVDD@5" pad="18"/>
<connect gate="G$1" pin="AVDD@6" pad="19"/>
<connect gate="G$1" pin="AVDD@7" pad="25"/>
<connect gate="G$1" pin="AVDD@8" pad="27"/>
<connect gate="G$1" pin="AVDD@9" pad="29"/>
<connect gate="G$1" pin="CLKMODESELCT" pad="11"/>
<connect gate="G$1" pin="CRYSTAL_OUT" pad="10"/>
<connect gate="G$1" pin="DACBP" pad="23"/>
<connect gate="G$1" pin="DAC_RSET" pad="24"/>
<connect gate="G$1" pin="DGND@1" pad="3"/>
<connect gate="G$1" pin="DGND@2" pad="33"/>
<connect gate="G$1" pin="DGND@3" pad="47"/>
<connect gate="G$1" pin="DGND@4" pad="42"/>
<connect gate="G$1" pin="DGND@5" pad="48"/>
<connect gate="G$1" pin="DVDD@1" pad="2"/>
<connect gate="G$1" pin="DVDD@2" pad="34"/>
<connect gate="G$1" pin="DVDD_I/O" pad="43"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="I/O_UPDATE" pad="1"/>
<connect gate="G$1" pin="IOSYNC" pad="37"/>
<connect gate="G$1" pin="IOUT" pad="21"/>
<connect gate="G$1" pin="LOOP_FILTER" pad="12"/>
<connect gate="G$1" pin="OSK" pad="46"/>
<connect gate="G$1" pin="PWRDWNCTL" pad="35"/>
<connect gate="G$1" pin="REFCLK" pad="9"/>
<connect gate="G$1" pin="RESET" pad="36"/>
<connect gate="G$1" pin="SCLK" pad="40"/>
<connect gate="G$1" pin="SDIO" pad="41"/>
<connect gate="G$1" pin="SDO" pad="38"/>
<connect gate="G$1" pin="SYNC_CLK" pad="45"/>
<connect gate="G$1" pin="SYNC_IN" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD9951YSVZ"/>
<attribute name="OC_FARNELL" value="8398445"/>
<attribute name="OC_NEWARK" value="19M1019"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_21367" prefix="IC">
<description>&lt;b&gt;SHARC Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 26&lt;/i&gt;&lt;br&gt;
Source: 17303025021367_256ballSBGA_bsdl_PrA_0106.txt</description>
<gates>
<gate name="G$1" symbol="17303025021367_256BALLSBGA_BSDL_PRA_0106"/>
</gates>
<devices>
<device name="" package="BP-256">
<connects>
<connect gate="G$1" pin="ACK" pad="M1"/>
<connect gate="G$1" pin="ADDR0" pad="W19"/>
<connect gate="G$1" pin="ADDR1" pad="W17"/>
<connect gate="G$1" pin="ADDR10" pad="W13"/>
<connect gate="G$1" pin="ADDR11" pad="Y13"/>
<connect gate="G$1" pin="ADDR12" pad="W12"/>
<connect gate="G$1" pin="ADDR13" pad="W11"/>
<connect gate="G$1" pin="ADDR14" pad="W8"/>
<connect gate="G$1" pin="ADDR15" pad="W7"/>
<connect gate="G$1" pin="ADDR16" pad="W6"/>
<connect gate="G$1" pin="ADDR17" pad="W5"/>
<connect gate="G$1" pin="ADDR18" pad="Y4"/>
<connect gate="G$1" pin="ADDR19" pad="W3"/>
<connect gate="G$1" pin="ADDR2" pad="W18"/>
<connect gate="G$1" pin="ADDR20" pad="W4"/>
<connect gate="G$1" pin="ADDR21" pad="W2"/>
<connect gate="G$1" pin="ADDR22" pad="V1"/>
<connect gate="G$1" pin="ADDR23" pad="V2"/>
<connect gate="G$1" pin="ADDR3" pad="Y17"/>
<connect gate="G$1" pin="ADDR4" pad="W16"/>
<connect gate="G$1" pin="ADDR5" pad="W15"/>
<connect gate="G$1" pin="ADDR6" pad="Y16"/>
<connect gate="G$1" pin="ADDR7" pad="Y15"/>
<connect gate="G$1" pin="ADDR8" pad="W14"/>
<connect gate="G$1" pin="ADDR9" pad="Y14"/>
<connect gate="G$1" pin="AVDD" pad="W9"/>
<connect gate="G$1" pin="AVSS" pad="W10"/>
<connect gate="G$1" pin="BOOTCFG0" pad="B5"/>
<connect gate="G$1" pin="BOOTCFG1" pad="B6"/>
<connect gate="G$1" pin="CLKIN" pad="Y8"/>
<connect gate="G$1" pin="CLKOUT" pad="A17"/>
<connect gate="G$1" pin="CLK_CFG0" pad="A4"/>
<connect gate="G$1" pin="CLK_CFG1" pad="A5"/>
<connect gate="G$1" pin="DAI1" pad="A8"/>
<connect gate="G$1" pin="DAI10" pad="D1"/>
<connect gate="G$1" pin="DAI11" pad="E1"/>
<connect gate="G$1" pin="DAI12" pad="F2"/>
<connect gate="G$1" pin="DAI13" pad="G2"/>
<connect gate="G$1" pin="DAI14" pad="F1"/>
<connect gate="G$1" pin="DAI15" pad="G1"/>
<connect gate="G$1" pin="DAI16" pad="H2"/>
<connect gate="G$1" pin="DAI17" pad="H1"/>
<connect gate="G$1" pin="DAI18" pad="J2"/>
<connect gate="G$1" pin="DAI19" pad="J1"/>
<connect gate="G$1" pin="DAI2" pad="B9"/>
<connect gate="G$1" pin="DAI20" pad="K2"/>
<connect gate="G$1" pin="DAI3" pad="B8"/>
<connect gate="G$1" pin="DAI4" pad="A7"/>
<connect gate="G$1" pin="DAI5" pad="B1"/>
<connect gate="G$1" pin="DAI6" pad="D2"/>
<connect gate="G$1" pin="DAI7" pad="C2"/>
<connect gate="G$1" pin="DAI8" pad="E2"/>
<connect gate="G$1" pin="DAI9" pad="C1"/>
<connect gate="G$1" pin="DATA0" pad="U19"/>
<connect gate="G$1" pin="DATA1" pad="V19"/>
<connect gate="G$1" pin="DATA10" pad="N20"/>
<connect gate="G$1" pin="DATA11" pad="N19"/>
<connect gate="G$1" pin="DATA12" pad="M19"/>
<connect gate="G$1" pin="DATA13" pad="M20"/>
<connect gate="G$1" pin="DATA14" pad="L20"/>
<connect gate="G$1" pin="DATA15" pad="L19"/>
<connect gate="G$1" pin="DATA16" pad="K20"/>
<connect gate="G$1" pin="DATA17" pad="J20"/>
<connect gate="G$1" pin="DATA18" pad="H20"/>
<connect gate="G$1" pin="DATA19" pad="H19"/>
<connect gate="G$1" pin="DATA2" pad="U20"/>
<connect gate="G$1" pin="DATA20" pad="G20"/>
<connect gate="G$1" pin="DATA21" pad="F20"/>
<connect gate="G$1" pin="DATA22" pad="G19"/>
<connect gate="G$1" pin="DATA23" pad="E20"/>
<connect gate="G$1" pin="DATA24" pad="D20"/>
<connect gate="G$1" pin="DATA25" pad="E19"/>
<connect gate="G$1" pin="DATA26" pad="D19"/>
<connect gate="G$1" pin="DATA27" pad="C19"/>
<connect gate="G$1" pin="DATA28" pad="B19"/>
<connect gate="G$1" pin="DATA29" pad="B18"/>
<connect gate="G$1" pin="DATA3" pad="V20"/>
<connect gate="G$1" pin="DATA30" pad="B17"/>
<connect gate="G$1" pin="DATA31" pad="A18"/>
<connect gate="G$1" pin="DATA4" pad="T20"/>
<connect gate="G$1" pin="DATA5" pad="T19"/>
<connect gate="G$1" pin="DATA6" pad="R19"/>
<connect gate="G$1" pin="DATA7" pad="R20"/>
<connect gate="G$1" pin="DATA8" pad="P19"/>
<connect gate="G$1" pin="DATA9" pad="P20"/>
<connect gate="G$1" pin="DPI1" pad="B15"/>
<connect gate="G$1" pin="DPI10" pad="A11"/>
<connect gate="G$1" pin="DPI11" pad="B11"/>
<connect gate="G$1" pin="DPI12" pad="A10"/>
<connect gate="G$1" pin="DPI13" pad="B10"/>
<connect gate="G$1" pin="DPI14" pad="A9"/>
<connect gate="G$1" pin="DPI2" pad="A16"/>
<connect gate="G$1" pin="DPI3" pad="A15"/>
<connect gate="G$1" pin="DPI4" pad="B14"/>
<connect gate="G$1" pin="DPI5" pad="B13"/>
<connect gate="G$1" pin="DPI6" pad="A14"/>
<connect gate="G$1" pin="DPI7" pad="A13"/>
<connect gate="G$1" pin="DPI8" pad="B12"/>
<connect gate="G$1" pin="DPI9" pad="A12"/>
<connect gate="G$1" pin="EMU_B" pad="A6"/>
<connect gate="G$1" pin="FLAG0" pad="K1"/>
<connect gate="G$1" pin="FLAG1" pad="L2"/>
<connect gate="G$1" pin="FLAG2" pad="L1"/>
<connect gate="G$1" pin="FLAG3" pad="M2"/>
<connect gate="G$1" pin="GND@0" pad="C3"/>
<connect gate="G$1" pin="GND@1" pad="C5"/>
<connect gate="G$1" pin="GND@10" pad="D5"/>
<connect gate="G$1" pin="GND@11" pad="D8"/>
<connect gate="G$1" pin="GND@12" pad="D11"/>
<connect gate="G$1" pin="GND@13" pad="D14"/>
<connect gate="G$1" pin="GND@14" pad="D16"/>
<connect gate="G$1" pin="GND@15" pad="D18"/>
<connect gate="G$1" pin="GND@16" pad="E17"/>
<connect gate="G$1" pin="GND@17" pad="E18"/>
<connect gate="G$1" pin="GND@18" pad="F3"/>
<connect gate="G$1" pin="GND@19" pad="F4"/>
<connect gate="G$1" pin="GND@2" pad="C6"/>
<connect gate="G$1" pin="GND@20" pad="F18"/>
<connect gate="G$1" pin="GND@21" pad="G3"/>
<connect gate="G$1" pin="GND@22" pad="H18"/>
<connect gate="G$1" pin="GND@23" pad="J3"/>
<connect gate="G$1" pin="GND@24" pad="J4"/>
<connect gate="G$1" pin="GND@25" pad="J17"/>
<connect gate="G$1" pin="GND@26" pad="J18"/>
<connect gate="G$1" pin="GND@27" pad="K3"/>
<connect gate="G$1" pin="GND@28" pad="M3"/>
<connect gate="G$1" pin="GND@29" pad="M4"/>
<connect gate="G$1" pin="GND@3" pad="C8"/>
<connect gate="G$1" pin="GND@30" pad="M18"/>
<connect gate="G$1" pin="GND@31" pad="N3"/>
<connect gate="G$1" pin="GND@32" pad="N17"/>
<connect gate="G$1" pin="GND@33" pad="N18"/>
<connect gate="G$1" pin="GND@34" pad="R3"/>
<connect gate="G$1" pin="GND@35" pad="R4"/>
<connect gate="G$1" pin="GND@36" pad="R18"/>
<connect gate="G$1" pin="GND@37" pad="T3"/>
<connect gate="G$1" pin="GND@38" pad="T17"/>
<connect gate="G$1" pin="GND@39" pad="T18"/>
<connect gate="G$1" pin="GND@4" pad="C9"/>
<connect gate="G$1" pin="GND@40" pad="U4"/>
<connect gate="G$1" pin="GND@41" pad="U6"/>
<connect gate="G$1" pin="GND@42" pad="U10"/>
<connect gate="G$1" pin="GND@43" pad="V4"/>
<connect gate="G$1" pin="GND@44" pad="V5"/>
<connect gate="G$1" pin="GND@45" pad="V6"/>
<connect gate="G$1" pin="GND@46" pad="V7"/>
<connect gate="G$1" pin="GND@47" pad="V9"/>
<connect gate="G$1" pin="GND@48" pad="V10"/>
<connect gate="G$1" pin="GND@49" pad="V11"/>
<connect gate="G$1" pin="GND@5" pad="C11"/>
<connect gate="G$1" pin="GND@50" pad="V14"/>
<connect gate="G$1" pin="GND@51" pad="V16"/>
<connect gate="G$1" pin="GND@52" pad="V17"/>
<connect gate="G$1" pin="GND@53" pad="V18"/>
<connect gate="G$1" pin="GND@54" pad="W1"/>
<connect gate="G$1" pin="GND@55" pad="Y1"/>
<connect gate="G$1" pin="GND@56" pad="Y18"/>
<connect gate="G$1" pin="GND@57" pad="Y19"/>
<connect gate="G$1" pin="GND@6" pad="C12"/>
<connect gate="G$1" pin="GND@7" pad="C14"/>
<connect gate="G$1" pin="GND@8" pad="C15"/>
<connect gate="G$1" pin="GND@9" pad="D3"/>
<connect gate="G$1" pin="GND_0" pad="K19"/>
<connect gate="G$1" pin="GND_1" pad="J19"/>
<connect gate="G$1" pin="GND_2" pad="F19"/>
<connect gate="G$1" pin="IOVDD@0" pad="C4"/>
<connect gate="G$1" pin="IOVDD@1" pad="D4"/>
<connect gate="G$1" pin="IOVDD@10" pad="K4"/>
<connect gate="G$1" pin="IOVDD@11" pad="M17"/>
<connect gate="G$1" pin="IOVDD@12" pad="N4"/>
<connect gate="G$1" pin="IOVDD@13" pad="R17"/>
<connect gate="G$1" pin="IOVDD@14" pad="T4"/>
<connect gate="G$1" pin="IOVDD@15" pad="U5"/>
<connect gate="G$1" pin="IOVDD@16" pad="U7"/>
<connect gate="G$1" pin="IOVDD@17" pad="U9"/>
<connect gate="G$1" pin="IOVDD@18" pad="U11"/>
<connect gate="G$1" pin="IOVDD@19" pad="U13"/>
<connect gate="G$1" pin="IOVDD@2" pad="D6"/>
<connect gate="G$1" pin="IOVDD@20" pad="U14"/>
<connect gate="G$1" pin="IOVDD@21" pad="U16"/>
<connect gate="G$1" pin="IOVDD@22" pad="V13"/>
<connect gate="G$1" pin="IOVDD@3" pad="D9"/>
<connect gate="G$1" pin="IOVDD@4" pad="D12"/>
<connect gate="G$1" pin="IOVDD@5" pad="D15"/>
<connect gate="G$1" pin="IOVDD@6" pad="D17"/>
<connect gate="G$1" pin="IOVDD@7" pad="F17"/>
<connect gate="G$1" pin="IOVDD@8" pad="G4"/>
<connect gate="G$1" pin="IOVDD@9" pad="H17"/>
<connect gate="G$1" pin="MS0_B" pad="U1"/>
<connect gate="G$1" pin="MS1_B" pad="U2"/>
<connect gate="G$1" pin="NC0" pad="A1"/>
<connect gate="G$1" pin="NC1" pad="A19"/>
<connect gate="G$1" pin="NC2" pad="A20"/>
<connect gate="G$1" pin="NC3" pad="B20"/>
<connect gate="G$1" pin="NC4" pad="W20"/>
<connect gate="G$1" pin="NC5" pad="Y2"/>
<connect gate="G$1" pin="NC6" pad="Y3"/>
<connect gate="G$1" pin="NC7" pad="Y9"/>
<connect gate="G$1" pin="NC8" pad="Y10"/>
<connect gate="G$1" pin="NC9" pad="Y20"/>
<connect gate="G$1" pin="NC_1" pad="Y12"/>
<connect gate="G$1" pin="NC_2" pad="Y11"/>
<connect gate="G$1" pin="NC_3" pad="Y6"/>
<connect gate="G$1" pin="NC_4" pad="Y5"/>
<connect gate="G$1" pin="NC_5" pad="B2"/>
<connect gate="G$1" pin="NC_6" pad="C20"/>
<connect gate="G$1" pin="RD_B" pad="N1"/>
<connect gate="G$1" pin="RESET_B" pad="B16"/>
<connect gate="G$1" pin="SDA10" pad="P1"/>
<connect gate="G$1" pin="SDCAS_B" pad="T2"/>
<connect gate="G$1" pin="SDCKE" pad="T1"/>
<connect gate="G$1" pin="SDCLK0" pad="N2"/>
<connect gate="G$1" pin="SDRAS_B" pad="R2"/>
<connect gate="G$1" pin="SDWE_B" pad="R1"/>
<connect gate="G$1" pin="TCK" pad="B4"/>
<connect gate="G$1" pin="TDI" pad="A2"/>
<connect gate="G$1" pin="TDO" pad="B7"/>
<connect gate="G$1" pin="TMS" pad="A3"/>
<connect gate="G$1" pin="TRST" pad="B3"/>
<connect gate="G$1" pin="VDD@0" pad="C7"/>
<connect gate="G$1" pin="VDD@1" pad="C10"/>
<connect gate="G$1" pin="VDD@10" pad="E4"/>
<connect gate="G$1" pin="VDD@11" pad="G17"/>
<connect gate="G$1" pin="VDD@12" pad="G18"/>
<connect gate="G$1" pin="VDD@13" pad="H3"/>
<connect gate="G$1" pin="VDD@14" pad="H4"/>
<connect gate="G$1" pin="VDD@15" pad="K17"/>
<connect gate="G$1" pin="VDD@16" pad="K18"/>
<connect gate="G$1" pin="VDD@17" pad="L3"/>
<connect gate="G$1" pin="VDD@18" pad="L4"/>
<connect gate="G$1" pin="VDD@19" pad="L17"/>
<connect gate="G$1" pin="VDD@2" pad="C13"/>
<connect gate="G$1" pin="VDD@20" pad="L18"/>
<connect gate="G$1" pin="VDD@21" pad="P3"/>
<connect gate="G$1" pin="VDD@22" pad="P4"/>
<connect gate="G$1" pin="VDD@23" pad="P17"/>
<connect gate="G$1" pin="VDD@24" pad="P18"/>
<connect gate="G$1" pin="VDD@25" pad="U3"/>
<connect gate="G$1" pin="VDD@26" pad="U8"/>
<connect gate="G$1" pin="VDD@27" pad="U12"/>
<connect gate="G$1" pin="VDD@28" pad="U15"/>
<connect gate="G$1" pin="VDD@29" pad="U17"/>
<connect gate="G$1" pin="VDD@3" pad="C16"/>
<connect gate="G$1" pin="VDD@30" pad="U18"/>
<connect gate="G$1" pin="VDD@31" pad="V3"/>
<connect gate="G$1" pin="VDD@32" pad="V8"/>
<connect gate="G$1" pin="VDD@33" pad="V12"/>
<connect gate="G$1" pin="VDD@34" pad="V15"/>
<connect gate="G$1" pin="VDD@4" pad="C17"/>
<connect gate="G$1" pin="VDD@5" pad="C18"/>
<connect gate="G$1" pin="VDD@6" pad="D7"/>
<connect gate="G$1" pin="VDD@7" pad="D10"/>
<connect gate="G$1" pin="VDD@8" pad="D13"/>
<connect gate="G$1" pin="VDD@9" pad="E3"/>
<connect gate="G$1" pin="WR_B" pad="P2"/>
<connect gate="G$1" pin="XTAL" pad="Y7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_21367-208" prefix="IC">
<description>&lt;b&gt;SHARC Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 26&lt;/i&gt;&lt;br&gt;
Source: 71207126721367_208pinMQFP_bsdl_PrA_0106.txt</description>
<gates>
<gate name="G$1" symbol="21367_208MQFP"/>
</gates>
<devices>
<device name="" package="LQFP208">
<connects>
<connect gate="G$1" pin="ACK" pad="120"/>
<connect gate="G$1" pin="ADDR0" pad="56"/>
<connect gate="G$1" pin="ADDR1" pad="58"/>
<connect gate="G$1" pin="ADDR10" pad="70"/>
<connect gate="G$1" pin="ADDR11" pad="75"/>
<connect gate="G$1" pin="ADDR12" pad="76"/>
<connect gate="G$1" pin="ADDR13" pad="77"/>
<connect gate="G$1" pin="ADDR14" pad="88"/>
<connect gate="G$1" pin="ADDR15" pad="91"/>
<connect gate="G$1" pin="ADDR16" pad="92"/>
<connect gate="G$1" pin="ADDR17" pad="93"/>
<connect gate="G$1" pin="ADDR18" pad="94"/>
<connect gate="G$1" pin="ADDR19" pad="97"/>
<connect gate="G$1" pin="ADDR2" pad="57"/>
<connect gate="G$1" pin="ADDR20" pad="98"/>
<connect gate="G$1" pin="ADDR21" pad="99"/>
<connect gate="G$1" pin="ADDR22" pad="101"/>
<connect gate="G$1" pin="ADDR23" pad="100"/>
<connect gate="G$1" pin="ADDR3" pad="60"/>
<connect gate="G$1" pin="ADDR4" pad="59"/>
<connect gate="G$1" pin="ADDR5" pad="61"/>
<connect gate="G$1" pin="ADDR6" pad="66"/>
<connect gate="G$1" pin="ADDR7" pad="67"/>
<connect gate="G$1" pin="ADDR8" pad="68"/>
<connect gate="G$1" pin="ADDR9" pad="69"/>
<connect gate="G$1" pin="AVDD" pad="81"/>
<connect gate="G$1" pin="AVSS" pad="80"/>
<connect gate="G$1" pin="BOOTCFG0" pad="170"/>
<connect gate="G$1" pin="BOOTCFG1" pad="173"/>
<connect gate="G$1" pin="CLKIN" pad="83"/>
<connect gate="G$1" pin="CLKOUT" pad="201"/>
<connect gate="G$1" pin="CLK_CFG0" pad="169"/>
<connect gate="G$1" pin="CLK_CFG1" pad="171"/>
<connect gate="G$1" pin="DAI1" pad="178"/>
<connect gate="G$1" pin="DAI10" pad="144"/>
<connect gate="G$1" pin="DAI11" pad="143"/>
<connect gate="G$1" pin="DAI12" pad="137"/>
<connect gate="G$1" pin="DAI13" pad="136"/>
<connect gate="G$1" pin="DAI14" pad="135"/>
<connect gate="G$1" pin="DAI15" pad="134"/>
<connect gate="G$1" pin="DAI16" pad="133"/>
<connect gate="G$1" pin="DAI17" pad="132"/>
<connect gate="G$1" pin="DAI18" pad="131"/>
<connect gate="G$1" pin="DAI19" pad="130"/>
<connect gate="G$1" pin="DAI2" pad="176"/>
<connect gate="G$1" pin="DAI20" pad="125"/>
<connect gate="G$1" pin="DAI3" pad="177"/>
<connect gate="G$1" pin="DAI4" pad="175"/>
<connect gate="G$1" pin="DAI5" pad="149"/>
<connect gate="G$1" pin="DAI6" pad="147"/>
<connect gate="G$1" pin="DAI7" pad="148"/>
<connect gate="G$1" pin="DAI8" pad="145"/>
<connect gate="G$1" pin="DAI9" pad="146"/>
<connect gate="G$1" pin="DATA0" pad="48"/>
<connect gate="G$1" pin="DATA1" pad="49"/>
<connect gate="G$1" pin="DATA10" pad="36"/>
<connect gate="G$1" pin="DATA11" pad="35"/>
<connect gate="G$1" pin="DATA12" pad="30"/>
<connect gate="G$1" pin="DATA13" pad="29"/>
<connect gate="G$1" pin="DATA14" pad="28"/>
<connect gate="G$1" pin="DATA15" pad="27"/>
<connect gate="G$1" pin="DATA16" pad="26"/>
<connect gate="G$1" pin="DATA17" pad="21"/>
<connect gate="G$1" pin="DATA18" pad="18"/>
<connect gate="G$1" pin="DATA19" pad="17"/>
<connect gate="G$1" pin="DATA2" pad="46"/>
<connect gate="G$1" pin="DATA20" pad="14"/>
<connect gate="G$1" pin="DATA21" pad="13"/>
<connect gate="G$1" pin="DATA22" pad="12"/>
<connect gate="G$1" pin="DATA23" pad="9"/>
<connect gate="G$1" pin="DATA24" pad="8"/>
<connect gate="G$1" pin="DATA25" pad="7"/>
<connect gate="G$1" pin="DATA26" pad="6"/>
<connect gate="G$1" pin="DATA27" pad="3"/>
<connect gate="G$1" pin="DATA28" pad="2"/>
<connect gate="G$1" pin="DATA29" pad="207"/>
<connect gate="G$1" pin="DATA3" pad="47"/>
<connect gate="G$1" pin="DATA30" pad="205"/>
<connect gate="G$1" pin="DATA31" pad="206"/>
<connect gate="G$1" pin="DATA4" pad="44"/>
<connect gate="G$1" pin="DATA5" pad="45"/>
<connect gate="G$1" pin="DATA6" pad="40"/>
<connect gate="G$1" pin="DATA7" pad="39"/>
<connect gate="G$1" pin="DATA8" pad="38"/>
<connect gate="G$1" pin="DATA9" pad="37"/>
<connect gate="G$1" pin="DPI1" pad="199"/>
<connect gate="G$1" pin="DPI10" pad="187"/>
<connect gate="G$1" pin="DPI11" pad="186"/>
<connect gate="G$1" pin="DPI12" pad="185"/>
<connect gate="G$1" pin="DPI13" pad="184"/>
<connect gate="G$1" pin="DPI14" pad="183"/>
<connect gate="G$1" pin="DPI2" pad="200"/>
<connect gate="G$1" pin="DPI3" pad="198"/>
<connect gate="G$1" pin="DPI4" pad="197"/>
<connect gate="G$1" pin="DPI5" pad="196"/>
<connect gate="G$1" pin="DPI6" pad="195"/>
<connect gate="G$1" pin="DPI7" pad="190"/>
<connect gate="G$1" pin="DPI8" pad="189"/>
<connect gate="G$1" pin="DPI9" pad="188"/>
<connect gate="G$1" pin="EMU_B" pad="172"/>
<connect gate="G$1" pin="FLAG0" pad="124"/>
<connect gate="G$1" pin="FLAG1" pad="123"/>
<connect gate="G$1" pin="FLAG2" pad="122"/>
<connect gate="G$1" pin="FLAG3" pad="121"/>
<connect gate="G$1" pin="GND@0" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@10" pad="54"/>
<connect gate="G$1" pin="GND@11" pad="62"/>
<connect gate="G$1" pin="GND@12" pad="64"/>
<connect gate="G$1" pin="GND@13" pad="71"/>
<connect gate="G$1" pin="GND@14" pad="73"/>
<connect gate="G$1" pin="GND@15" pad="78"/>
<connect gate="G$1" pin="GND@16" pad="82"/>
<connect gate="G$1" pin="GND@17" pad="86"/>
<connect gate="G$1" pin="GND@18" pad="89"/>
<connect gate="G$1" pin="GND@19" pad="95"/>
<connect gate="G$1" pin="GND@2" pad="16"/>
<connect gate="G$1" pin="GND@20" pad="106"/>
<connect gate="G$1" pin="GND@21" pad="114"/>
<connect gate="G$1" pin="GND@22" pad="117"/>
<connect gate="G$1" pin="GND@23" pad="126"/>
<connect gate="G$1" pin="GND@24" pad="128"/>
<connect gate="G$1" pin="GND@25" pad="140"/>
<connect gate="G$1" pin="GND@26" pad="142"/>
<connect gate="G$1" pin="GND@27" pad="151"/>
<connect gate="G$1" pin="GND@28" pad="153"/>
<connect gate="G$1" pin="GND@29" pad="155"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="GND@30" pad="159"/>
<connect gate="G$1" pin="GND@31" pad="166"/>
<connect gate="G$1" pin="GND@32" pad="180"/>
<connect gate="G$1" pin="GND@33" pad="182"/>
<connect gate="G$1" pin="GND@34" pad="192"/>
<connect gate="G$1" pin="GND@35" pad="194"/>
<connect gate="G$1" pin="GND@36" pad="204"/>
<connect gate="G$1" pin="GND@4" pad="23"/>
<connect gate="G$1" pin="GND@5" pad="25"/>
<connect gate="G$1" pin="GND@6" pad="32"/>
<connect gate="G$1" pin="GND@7" pad="34"/>
<connect gate="G$1" pin="GND@8" pad="42"/>
<connect gate="G$1" pin="GND@9" pad="51"/>
<connect gate="G$1" pin="IOVDD@0" pad="5"/>
<connect gate="G$1" pin="IOVDD@1" pad="15"/>
<connect gate="G$1" pin="IOVDD@10" pad="96"/>
<connect gate="G$1" pin="IOVDD@11" pad="107"/>
<connect gate="G$1" pin="IOVDD@12" pad="115"/>
<connect gate="G$1" pin="IOVDD@13" pad="129"/>
<connect gate="G$1" pin="IOVDD@14" pad="139"/>
<connect gate="G$1" pin="IOVDD@15" pad="150"/>
<connect gate="G$1" pin="IOVDD@16" pad="179"/>
<connect gate="G$1" pin="IOVDD@17" pad="191"/>
<connect gate="G$1" pin="IOVDD@18" pad="203"/>
<connect gate="G$1" pin="IOVDD@2" pad="31"/>
<connect gate="G$1" pin="IOVDD@3" pad="41"/>
<connect gate="G$1" pin="IOVDD@4" pad="50"/>
<connect gate="G$1" pin="IOVDD@5" pad="55"/>
<connect gate="G$1" pin="IOVDD@6" pad="65"/>
<connect gate="G$1" pin="IOVDD@7" pad="74"/>
<connect gate="G$1" pin="IOVDD@8" pad="85"/>
<connect gate="G$1" pin="IOVDD@9" pad="90"/>
<connect gate="G$1" pin="MS0_B" pad="103"/>
<connect gate="G$1" pin="MS1_B" pad="102"/>
<connect gate="G$1" pin="RD_B" pad="119"/>
<connect gate="G$1" pin="RESET_B" pad="202"/>
<connect gate="G$1" pin="SDA10" pad="113"/>
<connect gate="G$1" pin="SDCAS_B" pad="108"/>
<connect gate="G$1" pin="SDCKE" pad="110"/>
<connect gate="G$1" pin="SDCLK0" pad="116"/>
<connect gate="G$1" pin="SDRAS_B" pad="109"/>
<connect gate="G$1" pin="SDWE_B" pad="111"/>
<connect gate="G$1" pin="TCK" pad="165"/>
<connect gate="G$1" pin="TDI" pad="163"/>
<connect gate="G$1" pin="TDO" pad="174"/>
<connect gate="G$1" pin="TMS" pad="168"/>
<connect gate="G$1" pin="TRST" pad="164"/>
<connect gate="G$1" pin="VDD@0" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="11"/>
<connect gate="G$1" pin="VDD@10" pad="72"/>
<connect gate="G$1" pin="VDD@11" pad="79"/>
<connect gate="G$1" pin="VDD@12" pad="87"/>
<connect gate="G$1" pin="VDD@13" pad="104"/>
<connect gate="G$1" pin="VDD@14" pad="105"/>
<connect gate="G$1" pin="VDD@15" pad="118"/>
<connect gate="G$1" pin="VDD@16" pad="127"/>
<connect gate="G$1" pin="VDD@17" pad="138"/>
<connect gate="G$1" pin="VDD@18" pad="141"/>
<connect gate="G$1" pin="VDD@19" pad="152"/>
<connect gate="G$1" pin="VDD@2" pad="19"/>
<connect gate="G$1" pin="VDD@20" pad="154"/>
<connect gate="G$1" pin="VDD@21" pad="156"/>
<connect gate="G$1" pin="VDD@22" pad="157"/>
<connect gate="G$1" pin="VDD@23" pad="158"/>
<connect gate="G$1" pin="VDD@24" pad="160"/>
<connect gate="G$1" pin="VDD@25" pad="161"/>
<connect gate="G$1" pin="VDD@26" pad="162"/>
<connect gate="G$1" pin="VDD@27" pad="167"/>
<connect gate="G$1" pin="VDD@28" pad="181"/>
<connect gate="G$1" pin="VDD@29" pad="193"/>
<connect gate="G$1" pin="VDD@3" pad="22"/>
<connect gate="G$1" pin="VDD@30" pad="208"/>
<connect gate="G$1" pin="VDD@4" pad="24"/>
<connect gate="G$1" pin="VDD@5" pad="33"/>
<connect gate="G$1" pin="VDD@6" pad="43"/>
<connect gate="G$1" pin="VDD@7" pad="52"/>
<connect gate="G$1" pin="VDD@8" pad="53"/>
<connect gate="G$1" pin="VDD@9" pad="63"/>
<connect gate="G$1" pin="WR_B" pad="112"/>
<connect gate="G$1" pin="XTAL" pad="84"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1776212"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADIS16209" prefix="IC">
<description>&lt;b&gt;High Accuracy, Dual-Axis Digital Inclinometer and Accelerometer&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADIS16209.pdf</description>
<gates>
<gate name="G$1" symbol="ADIS16209"/>
</gates>
<devices>
<device name="" package="LGA16">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="!RST" pad="9"/>
<connect gate="G$1" pin="AUXADC" pad="14"/>
<connect gate="G$1" pin="AUXDAC" pad="12"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DIO1" pad="5"/>
<connect gate="G$1" pin="DIO2" pad="6"/>
<connect gate="G$1" pin="DOUT" pad="2"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="SCLK" pad="1"/>
<connect gate="G$1" pin="VDD" pad="13"/>
<connect gate="G$1" pin="VREF" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADIS16209CCCZ"/>
<attribute name="OC_FARNELL" value="1607244"/>
<attribute name="OC_NEWARK" value="71M1609"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG1408YCPZ" prefix="IC">
<description>&lt;b&gt;4 Ohm RON, 8-Channel, ±15 V/+12 V/±5 V iCMOS Multiplexers&lt;/b&gt;&lt;p&gt;
Source: 8x ADG1408_1409.pdf</description>
<gates>
<gate name="G$1" symbol="ADG1408"/>
<gate name="P" symbol="PWR-VSS_GND_VDD_EXP"/>
</gates>
<devices>
<device name="" package="LFCSP16">
<connects>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="14"/>
<connect gate="G$1" pin="A2" pad="13"/>
<connect gate="G$1" pin="D" pad="6"/>
<connect gate="G$1" pin="EN" pad="16"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="3"/>
<connect gate="G$1" pin="S3" pad="4"/>
<connect gate="G$1" pin="S4" pad="5"/>
<connect gate="G$1" pin="S5" pad="10"/>
<connect gate="G$1" pin="S6" pad="9"/>
<connect gate="G$1" pin="S7" pad="8"/>
<connect gate="G$1" pin="S8" pad="7"/>
<connect gate="P" pin="EXP" pad="EXP"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VDD" pad="11"/>
<connect gate="P" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG1408YCPZ-REEL7"/>
<attribute name="OC_FARNELL" value="1438940"/>
<attribute name="OC_NEWARK" value="28M3585"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG1408YRUZ" prefix="IC">
<description>&lt;b&gt;4 Ohm RON, 8-Channel, ±15 V/+12 V/±5 V iCMOS Multiplexers&lt;/b&gt;&lt;p&gt;
Source: 8x ADG1408_1409.pdf</description>
<gates>
<gate name="G$1" symbol="ADG1408"/>
<gate name="P" symbol="PWR-VSS_GND_VDD"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="D" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="S3" pad="6"/>
<connect gate="G$1" pin="S4" pad="7"/>
<connect gate="G$1" pin="S5" pad="12"/>
<connect gate="G$1" pin="S6" pad="11"/>
<connect gate="G$1" pin="S7" pad="10"/>
<connect gate="G$1" pin="S8" pad="9"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG1408YRUZ"/>
<attribute name="OC_FARNELL" value="1438940"/>
<attribute name="OC_NEWARK" value="28M3586"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG1409YRUZ" prefix="IC">
<description>&lt;b&gt;4 Ohm RON, 4-Channel, ±15 V/+12 V/±5 V iCMOS Multiplexers&lt;/b&gt;&lt;p&gt;
Source: 8x ADG1408_1409.pdf</description>
<gates>
<gate name="G$1" symbol="ADG1409"/>
<gate name="P" symbol="PWR-VSS_GND_VDD"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DA" pad="8"/>
<connect gate="G$1" pin="DB" pad="9"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="S1A" pad="4"/>
<connect gate="G$1" pin="S1B" pad="13"/>
<connect gate="G$1" pin="S2A" pad="5"/>
<connect gate="G$1" pin="S2B" pad="12"/>
<connect gate="G$1" pin="S3A" pad="6"/>
<connect gate="G$1" pin="S3B" pad="11"/>
<connect gate="G$1" pin="S4A" pad="7"/>
<connect gate="G$1" pin="S4B" pad="10"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG1409YRUZ"/>
<attribute name="OC_FARNELL" value="1438941"/>
<attribute name="OC_NEWARK" value="55M3850"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG1409YCPZ" prefix="IC">
<description>&lt;b&gt;4 Ohm RON, 4-Channel, ±15 V/+12 V/±5 V iCMOS Multiplexers&lt;/b&gt;&lt;p&gt;
Source: 8x ADG1408_1409.pdf</description>
<gates>
<gate name="G$1" symbol="ADG1409"/>
<gate name="P" symbol="PWR-VSS_GND_VDD_EXP"/>
</gates>
<devices>
<device name="" package="LFCSP16">
<connects>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="14"/>
<connect gate="G$1" pin="DA" pad="6"/>
<connect gate="G$1" pin="DB" pad="7"/>
<connect gate="G$1" pin="EN" pad="16"/>
<connect gate="G$1" pin="S1A" pad="2"/>
<connect gate="G$1" pin="S1B" pad="11"/>
<connect gate="G$1" pin="S2A" pad="3"/>
<connect gate="G$1" pin="S2B" pad="10"/>
<connect gate="G$1" pin="S3A" pad="4"/>
<connect gate="G$1" pin="S3B" pad="9"/>
<connect gate="G$1" pin="S4A" pad="5"/>
<connect gate="G$1" pin="S4B" pad="8"/>
<connect gate="P" pin="EXP" pad="EXP"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="VDD" pad="12"/>
<connect gate="P" pin="VSS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG1409YCPZ-REEL7"/>
<attribute name="OC_FARNELL" value="1438941"/>
<attribute name="OC_NEWARK" value="46M5169"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG608" prefix="IC">
<description>&lt;b&gt;3 V/5 V, 8 Channel High Performance Analog Multiplexers&lt;/b&gt;&lt;p&gt;
Source: ADG608_609.pdf</description>
<gates>
<gate name="G$1" symbol="ADG1408"/>
<gate name="P" symbol="PWR-VSS_GND_VDD"/>
</gates>
<devices>
<device name="RU" package="TSSOP16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="D" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="S3" pad="6"/>
<connect gate="G$1" pin="S4" pad="7"/>
<connect gate="G$1" pin="S5" pad="12"/>
<connect gate="G$1" pin="S6" pad="11"/>
<connect gate="G$1" pin="S7" pad="10"/>
<connect gate="G$1" pin="S8" pad="9"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG608BRU"/>
<attribute name="OC_FARNELL" value="1465227"/>
<attribute name="OC_NEWARK" value="16F6552"/>
</technology>
</technologies>
</device>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="D" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="S3" pad="6"/>
<connect gate="G$1" pin="S4" pad="7"/>
<connect gate="G$1" pin="S5" pad="12"/>
<connect gate="G$1" pin="S6" pad="11"/>
<connect gate="G$1" pin="S7" pad="10"/>
<connect gate="G$1" pin="S8" pad="9"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG608BNZ"/>
<attribute name="OC_FARNELL" value="1438944"/>
<attribute name="OC_NEWARK" value="15P0383"/>
</technology>
</technologies>
</device>
<device name="R" package="SOIC16N">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="D" pad="8"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="S1" pad="4"/>
<connect gate="G$1" pin="S2" pad="5"/>
<connect gate="G$1" pin="S3" pad="6"/>
<connect gate="G$1" pin="S4" pad="7"/>
<connect gate="G$1" pin="S5" pad="12"/>
<connect gate="G$1" pin="S6" pad="11"/>
<connect gate="G$1" pin="S7" pad="10"/>
<connect gate="G$1" pin="S8" pad="9"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG608BR"/>
<attribute name="OC_FARNELL" value="1438944"/>
<attribute name="OC_NEWARK" value="09B7118"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG609" prefix="IC">
<description>&lt;b&gt;3 V/5 V, 4 Channel High Performance Analog Multiplexers&lt;/b&gt;&lt;p&gt;
Source: ADG608_609.pdf</description>
<gates>
<gate name="G$1" symbol="ADG1409"/>
<gate name="P" symbol="PWR-VSS_GND_VDD"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DA" pad="8"/>
<connect gate="G$1" pin="DB" pad="9"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="S1A" pad="4"/>
<connect gate="G$1" pin="S1B" pad="13"/>
<connect gate="G$1" pin="S2A" pad="5"/>
<connect gate="G$1" pin="S2B" pad="12"/>
<connect gate="G$1" pin="S3A" pad="6"/>
<connect gate="G$1" pin="S3B" pad="11"/>
<connect gate="G$1" pin="S4A" pad="7"/>
<connect gate="G$1" pin="S4B" pad="10"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG609BN"/>
<attribute name="OC_FARNELL" value="1438945"/>
<attribute name="OC_NEWARK" value="66F3790"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DA" pad="8"/>
<connect gate="G$1" pin="DB" pad="9"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="S1A" pad="4"/>
<connect gate="G$1" pin="S1B" pad="13"/>
<connect gate="G$1" pin="S2A" pad="5"/>
<connect gate="G$1" pin="S2B" pad="12"/>
<connect gate="G$1" pin="S3A" pad="6"/>
<connect gate="G$1" pin="S3B" pad="11"/>
<connect gate="G$1" pin="S4A" pad="7"/>
<connect gate="G$1" pin="S4B" pad="10"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG609BRUZ"/>
<attribute name="OC_FARNELL" value="1438945"/>
<attribute name="OC_NEWARK" value="19M8664"/>
</technology>
</technologies>
</device>
<device name="R" package="SOIC16N">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DA" pad="8"/>
<connect gate="G$1" pin="DB" pad="9"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="S1A" pad="4"/>
<connect gate="G$1" pin="S1B" pad="13"/>
<connect gate="G$1" pin="S2A" pad="5"/>
<connect gate="G$1" pin="S2B" pad="12"/>
<connect gate="G$1" pin="S3A" pad="6"/>
<connect gate="G$1" pin="S3B" pad="11"/>
<connect gate="G$1" pin="S4A" pad="7"/>
<connect gate="G$1" pin="S4B" pad="10"/>
<connect gate="P" pin="GND" pad="15"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG609BRZ"/>
<attribute name="OC_FARNELL" value="1438945"/>
<attribute name="OC_NEWARK" value="15P0386"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG658" prefix="IC">
<description>&lt;b&gt;+3 V/+5 V/±5 V CMOS 8-Channel Analog Multiplexers&lt;/b&gt;&lt;p&gt;
Source: ADG658_659.pdf</description>
<gates>
<gate name="P" symbol="PWR-VSS_GND_VDD"/>
<gate name="G$1" symbol="ADG658"/>
</gates>
<devices>
<device name="RU" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!EN" pad="6"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="S1" pad="13"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="15"/>
<connect gate="G$1" pin="S4" pad="12"/>
<connect gate="G$1" pin="S5" pad="1"/>
<connect gate="G$1" pin="S6" pad="5"/>
<connect gate="G$1" pin="S7" pad="2"/>
<connect gate="G$1" pin="S8" pad="4"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG658YRUZ"/>
<attribute name="OC_FARNELL" value="1438947"/>
<attribute name="OC_NEWARK" value="19M8665"/>
</technology>
</technologies>
</device>
<device name="CP" package="LFCSP16">
<connects>
<connect gate="G$1" pin="!EN" pad="4"/>
<connect gate="G$1" pin="A0" pad="9"/>
<connect gate="G$1" pin="A1" pad="8"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="S1" pad="11"/>
<connect gate="G$1" pin="S2" pad="12"/>
<connect gate="G$1" pin="S3" pad="13"/>
<connect gate="G$1" pin="S4" pad="10"/>
<connect gate="G$1" pin="S5" pad="15"/>
<connect gate="G$1" pin="S6" pad="3"/>
<connect gate="G$1" pin="S7" pad="16"/>
<connect gate="G$1" pin="S8" pad="2"/>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG658YCP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="87H9636"/>
</technology>
</technologies>
</device>
<device name="RQ" package="QSOP16">
<connects>
<connect gate="G$1" pin="!EN" pad="6"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="S1" pad="13"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="S3" pad="15"/>
<connect gate="G$1" pin="S4" pad="12"/>
<connect gate="G$1" pin="S5" pad="1"/>
<connect gate="G$1" pin="S6" pad="5"/>
<connect gate="G$1" pin="S7" pad="2"/>
<connect gate="G$1" pin="S8" pad="4"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG658YRQ-REEL7"/>
<attribute name="OC_FARNELL" value="1438947"/>
<attribute name="OC_NEWARK" value="59K1455"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG659" prefix="IC">
<description>&lt;b&gt;+3 V/+5 V/±5 V CMOS 4-Channel Analog Multiplexers&lt;/b&gt;&lt;p&gt;
Source: ADG658_659.pdf</description>
<gates>
<gate name="G$1" symbol="ADG659"/>
<gate name="P" symbol="PWR-VSS_GND_VDD"/>
</gates>
<devices>
<device name="CP" package="LFCSP16">
<connects>
<connect gate="G$1" pin="!EN" pad="4"/>
<connect gate="G$1" pin="A0" pad="8"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="DA" pad="11"/>
<connect gate="G$1" pin="DB" pad="1"/>
<connect gate="G$1" pin="S1A" pad="10"/>
<connect gate="G$1" pin="S1B" pad="15"/>
<connect gate="G$1" pin="S2A" pad="12"/>
<connect gate="G$1" pin="S2B" pad="3"/>
<connect gate="G$1" pin="S3A" pad="13"/>
<connect gate="G$1" pin="S3B" pad="16"/>
<connect gate="G$1" pin="S4A" pad="9"/>
<connect gate="G$1" pin="S4B" pad="2"/>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG659YCPZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="74R5857"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!EN" pad="6"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="DA" pad="13"/>
<connect gate="G$1" pin="DB" pad="3"/>
<connect gate="G$1" pin="S1A" pad="12"/>
<connect gate="G$1" pin="S1B" pad="1"/>
<connect gate="G$1" pin="S2A" pad="14"/>
<connect gate="G$1" pin="S2B" pad="5"/>
<connect gate="G$1" pin="S3A" pad="15"/>
<connect gate="G$1" pin="S3B" pad="2"/>
<connect gate="G$1" pin="S4A" pad="11"/>
<connect gate="G$1" pin="S4B" pad="4"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG659YRU-REEL7"/>
<attribute name="OC_FARNELL" value="1438948"/>
<attribute name="OC_NEWARK" value="50H3058"/>
</technology>
</technologies>
</device>
<device name="RQ" package="QSOP16">
<connects>
<connect gate="G$1" pin="!EN" pad="6"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="DA" pad="13"/>
<connect gate="G$1" pin="DB" pad="3"/>
<connect gate="G$1" pin="S1A" pad="12"/>
<connect gate="G$1" pin="S1B" pad="1"/>
<connect gate="G$1" pin="S2A" pad="14"/>
<connect gate="G$1" pin="S2B" pad="5"/>
<connect gate="G$1" pin="S3A" pad="15"/>
<connect gate="G$1" pin="S3B" pad="2"/>
<connect gate="G$1" pin="S4A" pad="11"/>
<connect gate="G$1" pin="S4B" pad="4"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VSS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG659YRQ"/>
<attribute name="OC_FARNELL" value="1465237"/>
<attribute name="OC_NEWARK" value="59K1460"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSM2165" prefix="IC">
<description>&lt;b&gt;Microphone Preamplifier with Variable Compression and Noise Gating&lt;/b&gt; &lt;font color="red"&gt;OBSOLETE&lt;/font&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets_obsolete/564647885SSM2165.pdf</description>
<gates>
<gate name="G$1" symbol="SSM2165"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="AVGCAP" pad="5"/>
<connect gate="G$1" pin="BUFOUT" pad="3"/>
<connect gate="G$1" pin="COMP" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VCAIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SO8">
<connects>
<connect gate="G$1" pin="AVGCAP" pad="5"/>
<connect gate="G$1" pin="BUFOUT" pad="3"/>
<connect gate="G$1" pin="COMP" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="VCAIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSM2166" prefix="IC">
<description>&lt;b&gt;Microphone Preamplifier with Variable Compression and Noise Gating&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/SSM2166.pdf</description>
<gates>
<gate name="G$1" symbol="SSM2166"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="G$1" pin="+IN" pad="7"/>
<connect gate="G$1" pin="-IN" pad="6"/>
<connect gate="G$1" pin="AVGCAP" pad="8"/>
<connect gate="G$1" pin="BUFOUT" pad="5"/>
<connect gate="G$1" pin="COMP" pad="10"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NOIS_GATE_SET" pad="9"/>
<connect gate="G$1" pin="POWER_DOWN" pad="12"/>
<connect gate="G$1" pin="ROTATION_POINT_SET" pad="11"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="VCAIN" pad="3"/>
<connect gate="G$1" pin="VCAR" pad="4"/>
<connect gate="G$1" pin="VCA_GAIN_ADJ" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SO14">
<connects>
<connect gate="G$1" pin="+IN" pad="7"/>
<connect gate="G$1" pin="-IN" pad="6"/>
<connect gate="G$1" pin="AVGCAP" pad="8"/>
<connect gate="G$1" pin="BUFOUT" pad="5"/>
<connect gate="G$1" pin="COMP" pad="10"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NOIS_GATE_SET" pad="9"/>
<connect gate="G$1" pin="POWER_DOWN" pad="12"/>
<connect gate="G$1" pin="ROTATION_POINT_SET" pad="11"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="VCAIN" pad="3"/>
<connect gate="G$1" pin="VCAR" pad="4"/>
<connect gate="G$1" pin="VCA_GAIN_ADJ" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="SSM2166S-REEL"/>
<attribute name="OC_FARNELL" value="1424669"/>
<attribute name="OC_NEWARK" value="13B4818"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSM2167" prefix="IC">
<description>&lt;b&gt;Low Voltage Microphone Preamplifier with Variable Compression and Noise Gating&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com .. SSM2167.pdf</description>
<gates>
<gate name="G$1" symbol="SSM2167"/>
</gates>
<devices>
<device name="" package="SO10">
<connects>
<connect gate="G$1" pin="!SHUTDOWN" pad="3"/>
<connect gate="G$1" pin="AVG_CAP" pad="6"/>
<connect gate="G$1" pin="BUFOUT" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUTPUT" pad="9"/>
<connect gate="G$1" pin="RCOMP" pad="8"/>
<connect gate="G$1" pin="RGATE" pad="7"/>
<connect gate="G$1" pin="VCAIN" pad="2"/>
<connect gate="G$1" pin="VDD" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SSM2167Z-EVAL"/>
<attribute name="OC_FARNELL" value="1424672"/>
<attribute name="OC_NEWARK" value="65M4647"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1836" prefix="IC">
<description>&lt;b&gt;Multichannel 96 kHz Codec&lt;/b&gt;&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 32&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1836.pdf</description>
<gates>
<gate name="G$1" symbol="AD1836"/>
</gates>
<devices>
<device name="" package="PQFP52">
<connects>
<connect gate="G$1" pin="ABCLK" pad="43"/>
<connect gate="G$1" pin="ADC1INLN" pad="17"/>
<connect gate="G$1" pin="ADC1INLP" pad="16"/>
<connect gate="G$1" pin="ADC1INRN" pad="19"/>
<connect gate="G$1" pin="ADC1INRP" pad="18"/>
<connect gate="G$1" pin="ADC2INL+/CAPL2" pad="20"/>
<connect gate="G$1" pin="ADC2INL-/CAPL1" pad="21"/>
<connect gate="G$1" pin="ADC2INL1" pad="22"/>
<connect gate="G$1" pin="ADC2INL2" pad="23"/>
<connect gate="G$1" pin="ADC2INR+/CAPR2" pad="27"/>
<connect gate="G$1" pin="ADC2INR-/CAPR1" pad="26"/>
<connect gate="G$1" pin="ADC2INR1" pad="25"/>
<connect gate="G$1" pin="ADC2INR2" pad="24"/>
<connect gate="G$1" pin="AGND" pad="11"/>
<connect gate="G$1" pin="AGND@1" pad="14"/>
<connect gate="G$1" pin="AGND@2" pad="28"/>
<connect gate="G$1" pin="AGND@3" pad="29"/>
<connect gate="G$1" pin="ALRCLK" pad="44"/>
<connect gate="G$1" pin="ASDATA1" pad="47"/>
<connect gate="G$1" pin="ASDATA2" pad="48"/>
<connect gate="G$1" pin="AVDD" pad="10"/>
<connect gate="G$1" pin="AVDD@1" pad="15"/>
<connect gate="G$1" pin="CCLK" pad="51"/>
<connect gate="G$1" pin="CDATA" pad="2"/>
<connect gate="G$1" pin="CLATCH" pad="50"/>
<connect gate="G$1" pin="COUT" pad="49"/>
<connect gate="G$1" pin="DBCLK" pad="37"/>
<connect gate="G$1" pin="DGND" pad="39"/>
<connect gate="G$1" pin="DGND@1" pad="52"/>
<connect gate="G$1" pin="DLRCLK" pad="36"/>
<connect gate="G$1" pin="DSDATA1" pad="38"/>
<connect gate="G$1" pin="DSDATA2" pad="41"/>
<connect gate="G$1" pin="DSDATA3" pad="42"/>
<connect gate="G$1" pin="DVDD" pad="1"/>
<connect gate="G$1" pin="DVDD@1" pad="40"/>
<connect gate="G$1" pin="FILTD" pad="12"/>
<connect gate="G$1" pin="FILTR" pad="13"/>
<connect gate="G$1" pin="MCLK" pad="45"/>
<connect gate="G$1" pin="ODVDD" pad="46"/>
<connect gate="G$1" pin="OUTLN1" pad="9"/>
<connect gate="G$1" pin="OUTLN2" pad="7"/>
<connect gate="G$1" pin="OUTLN3" pad="5"/>
<connect gate="G$1" pin="OUTLP1" pad="8"/>
<connect gate="G$1" pin="OUTLP2" pad="6"/>
<connect gate="G$1" pin="OUTLP3" pad="4"/>
<connect gate="G$1" pin="OUTRN1" pad="30"/>
<connect gate="G$1" pin="OUTRN2" pad="32"/>
<connect gate="G$1" pin="OUTRN3" pad="34"/>
<connect gate="G$1" pin="OUTRP1" pad="31"/>
<connect gate="G$1" pin="OUTRP2" pad="33"/>
<connect gate="G$1" pin="OUTRP3" pad="35"/>
<connect gate="G$1" pin="PD/RST" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD1836AASZ"/>
<attribute name="OC_FARNELL" value="8396558"/>
<attribute name="OC_NEWARK" value="59K3418"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUM1301" prefix="IC">
<description>&lt;b&gt;Triple-Channel Digital Isolators&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADuM1300_1301.pdf</description>
<gates>
<gate name="G$1" symbol="ADUM1301"/>
</gates>
<devices>
<device name="" package="SO-16W">
<connects>
<connect gate="G$1" pin="GND1@1" pad="2"/>
<connect gate="G$1" pin="GND1@2" pad="8"/>
<connect gate="G$1" pin="GND2@1" pad="15"/>
<connect gate="G$1" pin="GND2@2" pad="9"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="11"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VE1" pad="7"/>
<connect gate="G$1" pin="VE2" pad="10"/>
<connect gate="G$1" pin="VIA" pad="3"/>
<connect gate="G$1" pin="VIB" pad="4"/>
<connect gate="G$1" pin="VIC" pad="12"/>
<connect gate="G$1" pin="VOA" pad="14"/>
<connect gate="G$1" pin="VOB" pad="13"/>
<connect gate="G$1" pin="VOC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUM1301BRWZ"/>
<attribute name="OC_FARNELL" value="1465623"/>
<attribute name="OC_NEWARK" value="19M0757"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUM1300" prefix="IC">
<description>&lt;b&gt;Triple-Channel Digital Isolators&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADuM1300_1301.pdf</description>
<gates>
<gate name="G$1" symbol="ADUM1300"/>
</gates>
<devices>
<device name="" package="SO-16W">
<connects>
<connect gate="G$1" pin="GND1@1" pad="2"/>
<connect gate="G$1" pin="GND1@2" pad="8"/>
<connect gate="G$1" pin="GND2@1" pad="15"/>
<connect gate="G$1" pin="GND2@2" pad="9"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="7"/>
<connect gate="G$1" pin="NC@3" pad="11"/>
<connect gate="G$1" pin="VDD1" pad="1"/>
<connect gate="G$1" pin="VDD2" pad="16"/>
<connect gate="G$1" pin="VE2" pad="10"/>
<connect gate="G$1" pin="VIA" pad="3"/>
<connect gate="G$1" pin="VIB" pad="4"/>
<connect gate="G$1" pin="VIC" pad="5"/>
<connect gate="G$1" pin="VOA" pad="14"/>
<connect gate="G$1" pin="VOB" pad="13"/>
<connect gate="G$1" pin="VOC" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUM1300ARWZ"/>
<attribute name="OC_FARNELL" value="1465621"/>
<attribute name="OC_NEWARK" value="19M8751"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1877" prefix="IC">
<description>&lt;b&gt;Single-Supply 16-Bit Stereo ADC&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1877.pdf</description>
<gates>
<gate name="G$1" symbol="AD1877"/>
</gates>
<devices>
<device name="" package="SO-28R">
<connects>
<connect gate="G$1" pin="!MSBDLY" pad="22"/>
<connect gate="G$1" pin="!RESET" pad="23"/>
<connect gate="G$1" pin="384/!256" pad="8"/>
<connect gate="G$1" pin="AGND" pad="20"/>
<connect gate="G$1" pin="AGNDL" pad="13"/>
<connect gate="G$1" pin="AGNDR" pad="16"/>
<connect gate="G$1" pin="AVDD" pad="9"/>
<connect gate="G$1" pin="BCLK" pad="3"/>
<connect gate="G$1" pin="CAPL1" pad="11"/>
<connect gate="G$1" pin="CAPL2" pad="12"/>
<connect gate="G$1" pin="CAPR1" pad="18"/>
<connect gate="G$1" pin="CAPR2" pad="17"/>
<connect gate="G$1" pin="CLKIN" pad="28"/>
<connect gate="G$1" pin="DGND1" pad="5"/>
<connect gate="G$1" pin="DGND2" pad="24"/>
<connect gate="G$1" pin="DVDD1" pad="4"/>
<connect gate="G$1" pin="DVDD2" pad="25"/>
<connect gate="G$1" pin="L!R!CK" pad="1"/>
<connect gate="G$1" pin="R!L!JUST" pad="21"/>
<connect gate="G$1" pin="RDEDGE" pad="6"/>
<connect gate="G$1" pin="S/!M" pad="7"/>
<connect gate="G$1" pin="SOUT" pad="26"/>
<connect gate="G$1" pin="TAG" pad="27"/>
<connect gate="G$1" pin="VINL" pad="10"/>
<connect gate="G$1" pin="VINR" pad="19"/>
<connect gate="G$1" pin="VREFL" pad="14"/>
<connect gate="G$1" pin="VREFR" pad="15"/>
<connect gate="G$1" pin="WCLK" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD1877JRZ"/>
<attribute name="OC_FARNELL" value="1438337"/>
<attribute name="OC_NEWARK" value="12M8449"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1890" prefix="IC">
<description>&lt;b&gt;SamplePort Stereo Asynchronous Sample Rate Converters&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1890_1891.pdf</description>
<gates>
<gate name="G$1" symbol="AD1890"/>
</gates>
<devices>
<device name="JN" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="BCLK_I" pad="4"/>
<connect gate="G$1" pin="BCLK_O" pad="26"/>
<connect gate="G$1" pin="BKPOL_I" pad="10"/>
<connect gate="G$1" pin="BKPOL_O" pad="19"/>
<connect gate="G$1" pin="DATA_I" pad="3"/>
<connect gate="G$1" pin="DATA_O" pad="23"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="21"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GPDLYS" pad="1"/>
<connect gate="G$1" pin="L!R!_I" pad="6"/>
<connect gate="G$1" pin="L!R!_O" pad="24"/>
<connect gate="G$1" pin="MCLK" pad="2"/>
<connect gate="G$1" pin="MSBDLY_I" pad="12"/>
<connect gate="G$1" pin="MSBDLY_O" pad="17"/>
<connect gate="G$1" pin="MUTE_I" pad="15"/>
<connect gate="G$1" pin="MUTE_O" pad="16"/>
<connect gate="G$1" pin="N/C" pad="9"/>
<connect gate="G$1" pin="N/C@1" pad="20"/>
<connect gate="G$1" pin="SETLSLW" pad="28"/>
<connect gate="G$1" pin="TRGLR_I" pad="11"/>
<connect gate="G$1" pin="TRGLR_O" pad="18"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="22"/>
<connect gate="G$1" pin="WCLK_I" pad="5"/>
<connect gate="G$1" pin="WCLK_O" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="JP" package="PLCC28S">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="BCLK_I" pad="4"/>
<connect gate="G$1" pin="BCLK_O" pad="26"/>
<connect gate="G$1" pin="BKPOL_I" pad="10"/>
<connect gate="G$1" pin="BKPOL_O" pad="19"/>
<connect gate="G$1" pin="DATA_I" pad="3"/>
<connect gate="G$1" pin="DATA_O" pad="23"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="21"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="GPDLYS" pad="1"/>
<connect gate="G$1" pin="L!R!_I" pad="6"/>
<connect gate="G$1" pin="L!R!_O" pad="24"/>
<connect gate="G$1" pin="MCLK" pad="2"/>
<connect gate="G$1" pin="MSBDLY_I" pad="12"/>
<connect gate="G$1" pin="MSBDLY_O" pad="17"/>
<connect gate="G$1" pin="MUTE_I" pad="15"/>
<connect gate="G$1" pin="MUTE_O" pad="16"/>
<connect gate="G$1" pin="N/C" pad="9"/>
<connect gate="G$1" pin="N/C@1" pad="20"/>
<connect gate="G$1" pin="SETLSLW" pad="28"/>
<connect gate="G$1" pin="TRGLR_I" pad="11"/>
<connect gate="G$1" pin="TRGLR_O" pad="18"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="22"/>
<connect gate="G$1" pin="WCLK_I" pad="5"/>
<connect gate="G$1" pin="WCLK_O" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD1890JP"/>
<attribute name="OC_FARNELL" value="1464273"/>
<attribute name="OC_NEWARK" value="66F1855"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1891" prefix="IC">
<description>&lt;b&gt;SamplePort Stereo Asynchronous Sample Rate Converters&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1890_1891.pdf</description>
<gates>
<gate name="G$1" symbol="AD1891"/>
</gates>
<devices>
<device name="JN" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="BCLK_I" pad="4"/>
<connect gate="G$1" pin="BCLK_O" pad="26"/>
<connect gate="G$1" pin="BKPOL_I" pad="10"/>
<connect gate="G$1" pin="BKPOL_O" pad="19"/>
<connect gate="G$1" pin="DATA_I" pad="3"/>
<connect gate="G$1" pin="DATA_O" pad="23"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="21"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="L!R!_I" pad="6"/>
<connect gate="G$1" pin="L!R!_O" pad="24"/>
<connect gate="G$1" pin="MCLK" pad="2"/>
<connect gate="G$1" pin="MSBDLY_I" pad="12"/>
<connect gate="G$1" pin="MSBDLY_O" pad="17"/>
<connect gate="G$1" pin="MUTE_I" pad="15"/>
<connect gate="G$1" pin="MUTE_O" pad="16"/>
<connect gate="G$1" pin="N/C@1" pad="1"/>
<connect gate="G$1" pin="N/C@2" pad="9"/>
<connect gate="G$1" pin="N/C@3" pad="20"/>
<connect gate="G$1" pin="SETLSLW" pad="28"/>
<connect gate="G$1" pin="TRGLR_I" pad="11"/>
<connect gate="G$1" pin="TRGLR_O" pad="18"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="22"/>
<connect gate="G$1" pin="WCLK_I" pad="5"/>
<connect gate="G$1" pin="WCLK_O" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="JP" package="PLCC28S">
<connects>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="BCLK_I" pad="4"/>
<connect gate="G$1" pin="BCLK_O" pad="26"/>
<connect gate="G$1" pin="BKPOL_I" pad="10"/>
<connect gate="G$1" pin="BKPOL_O" pad="19"/>
<connect gate="G$1" pin="DATA_I" pad="3"/>
<connect gate="G$1" pin="DATA_O" pad="23"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="21"/>
<connect gate="G$1" pin="GND@3" pad="27"/>
<connect gate="G$1" pin="L!R!_I" pad="6"/>
<connect gate="G$1" pin="L!R!_O" pad="24"/>
<connect gate="G$1" pin="MCLK" pad="2"/>
<connect gate="G$1" pin="MSBDLY_I" pad="12"/>
<connect gate="G$1" pin="MSBDLY_O" pad="17"/>
<connect gate="G$1" pin="MUTE_I" pad="15"/>
<connect gate="G$1" pin="MUTE_O" pad="16"/>
<connect gate="G$1" pin="N/C@1" pad="1"/>
<connect gate="G$1" pin="N/C@2" pad="9"/>
<connect gate="G$1" pin="N/C@3" pad="20"/>
<connect gate="G$1" pin="SETLSLW" pad="28"/>
<connect gate="G$1" pin="TRGLR_I" pad="11"/>
<connect gate="G$1" pin="TRGLR_O" pad="18"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="22"/>
<connect gate="G$1" pin="WCLK_I" pad="5"/>
<connect gate="G$1" pin="WCLK_O" pad="25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1892" prefix="IC">
<description>&lt;b&gt;Integrated Digital Receiver/Rate Converter&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1892.pdf</description>
<gates>
<gate name="G$1" symbol="AD1892"/>
</gates>
<devices>
<device name="" package="SO-28R">
<connects>
<connect gate="G$1" pin="BCLK" pad="26"/>
<connect gate="G$1" pin="CA" pad="21"/>
<connect gate="G$1" pin="CB" pad="20"/>
<connect gate="G$1" pin="CC" pad="19"/>
<connect gate="G$1" pin="CCLK" pad="2"/>
<connect gate="G$1" pin="CD" pad="18"/>
<connect gate="G$1" pin="CE" pad="17"/>
<connect gate="G$1" pin="CON/PRO" pad="15"/>
<connect gate="G$1" pin="CS" pad="3"/>
<connect gate="G$1" pin="CSCLK" pad="16"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DVDD" pad="22"/>
<connect gate="G$1" pin="ERROR" pad="11"/>
<connect gate="G$1" pin="INT" pad="10"/>
<connect gate="G$1" pin="LRCLK" pad="25"/>
<connect gate="G$1" pin="MCLK" pad="28"/>
<connect gate="G$1" pin="MUTE" pad="27"/>
<connect gate="G$1" pin="NOSIG" pad="12"/>
<connect gate="G$1" pin="PD/RST" pad="1"/>
<connect gate="G$1" pin="QDFS" pad="6"/>
<connect gate="G$1" pin="RXN" pad="14"/>
<connect gate="G$1" pin="RXP" pad="13"/>
<connect gate="G$1" pin="SDATA" pad="24"/>
<connect gate="G$1" pin="SDI" pad="4"/>
<connect gate="G$1" pin="SDO" pad="5"/>
<connect gate="G$1" pin="SFCLK" pad="8"/>
<connect gate="G$1" pin="SYNC" pad="23"/>
<connect gate="G$1" pin="U/CBIT" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1953" prefix="IC">
<description>&lt;b&gt;SigmaDSP (TM) 3-Channel, 26-Bit Signal Processing DAC&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1953.pdf</description>
<gates>
<gate name="G$1" symbol="AD1953"/>
</gates>
<devices>
<device name="" package="QFP-7X7-48">
<connects>
<connect gate="G$1" pin="AGND" pad="23"/>
<connect gate="G$1" pin="AGND@1" pad="27"/>
<connect gate="G$1" pin="AGND@2" pad="31"/>
<connect gate="G$1" pin="AGND@3" pad="35"/>
<connect gate="G$1" pin="AUXDATA" pad="5"/>
<connect gate="G$1" pin="AVDD" pad="22"/>
<connect gate="G$1" pin="AVDD@1" pad="30"/>
<connect gate="G$1" pin="AVDD@2" pad="32"/>
<connect gate="G$1" pin="BCLK0" pad="16"/>
<connect gate="G$1" pin="BCLK1" pad="12"/>
<connect gate="G$1" pin="BCLK2" pad="9"/>
<connect gate="G$1" pin="BMUXO/TDMBC" pad="42"/>
<connect gate="G$1" pin="CCLK" pad="19"/>
<connect gate="G$1" pin="CDATA" pad="18"/>
<connect gate="G$1" pin="CLATCH" pad="20"/>
<connect gate="G$1" pin="COUT" pad="46"/>
<connect gate="G$1" pin="DCSOUT" pad="45"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="DGND@1" pad="48"/>
<connect gate="G$1" pin="DMUXO/TDMO" pad="41"/>
<connect gate="G$1" pin="DVDD" pad="7"/>
<connect gate="G$1" pin="FILTCAP" pad="39"/>
<connect gate="G$1" pin="LRCLK0" pad="17"/>
<connect gate="G$1" pin="LRCLK1" pad="14"/>
<connect gate="G$1" pin="LRCLK2" pad="10"/>
<connect gate="G$1" pin="LRMUXO/TDMFS" pad="43"/>
<connect gate="G$1" pin="MCLK0" pad="4"/>
<connect gate="G$1" pin="MCLK1" pad="3"/>
<connect gate="G$1" pin="MCLK2" pad="2"/>
<connect gate="G$1" pin="MCLKOUT" pad="47"/>
<connect gate="G$1" pin="MUTE" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="24"/>
<connect gate="G$1" pin="NC@2" pad="36"/>
<connect gate="G$1" pin="NC@3" pad="37"/>
<connect gate="G$1" pin="ODVDD" pad="44"/>
<connect gate="G$1" pin="RESETB" pad="21"/>
<connect gate="G$1" pin="SDATA0" pad="15"/>
<connect gate="G$1" pin="SDATA1" pad="11"/>
<connect gate="G$1" pin="SDATA2" pad="8"/>
<connect gate="G$1" pin="VOUTL+" pad="33"/>
<connect gate="G$1" pin="VOUTL-" pad="34"/>
<connect gate="G$1" pin="VOUTR+" pad="29"/>
<connect gate="G$1" pin="VOUTR-" pad="28"/>
<connect gate="G$1" pin="VOUTS+" pad="26"/>
<connect gate="G$1" pin="VOUTS-" pad="25"/>
<connect gate="G$1" pin="VREF" pad="38"/>
<connect gate="G$1" pin="ZEROFLAG" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD1953YSTZRL7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8457"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1954" prefix="IC">
<description>&lt;b&gt;SigmaDSP? 3-Channel, 26-Bit Signal Processing DAC&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1954.pdf</description>
<gates>
<gate name="G$1" symbol="AD1954"/>
</gates>
<devices>
<device name="" package="LFCSP48">
<connects>
<connect gate="G$1" pin="AGND" pad="23"/>
<connect gate="G$1" pin="AGND@1" pad="27"/>
<connect gate="G$1" pin="AGND@2" pad="31"/>
<connect gate="G$1" pin="AGND@3" pad="35"/>
<connect gate="G$1" pin="AVDD" pad="22"/>
<connect gate="G$1" pin="AVDD@1" pad="30"/>
<connect gate="G$1" pin="AVDD@2" pad="32"/>
<connect gate="G$1" pin="BCLK0" pad="16"/>
<connect gate="G$1" pin="BCLK1" pad="12"/>
<connect gate="G$1" pin="BCLK2" pad="9"/>
<connect gate="G$1" pin="BCLKOUT" pad="42"/>
<connect gate="G$1" pin="CCLK" pad="19"/>
<connect gate="G$1" pin="CDATA" pad="18"/>
<connect gate="G$1" pin="CLATCH" pad="20"/>
<connect gate="G$1" pin="COUT" pad="46"/>
<connect gate="G$1" pin="DCSOUT" pad="45"/>
<connect gate="G$1" pin="DEEMP/SDATA_AUX" pad="5"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="DGND@1" pad="48"/>
<connect gate="G$1" pin="DVDD" pad="7"/>
<connect gate="G$1" pin="FILTCAP" pad="39"/>
<connect gate="G$1" pin="LRCLK0" pad="17"/>
<connect gate="G$1" pin="LRCLK1" pad="14"/>
<connect gate="G$1" pin="LRCLK2" pad="10"/>
<connect gate="G$1" pin="LRCLKOUT" pad="43"/>
<connect gate="G$1" pin="MCLK0" pad="4"/>
<connect gate="G$1" pin="MCLK1" pad="3"/>
<connect gate="G$1" pin="MCLK2" pad="2"/>
<connect gate="G$1" pin="MCLKOUT" pad="47"/>
<connect gate="G$1" pin="MUTE" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="24"/>
<connect gate="G$1" pin="NC@2" pad="36"/>
<connect gate="G$1" pin="NC@3" pad="37"/>
<connect gate="G$1" pin="ODVDD" pad="44"/>
<connect gate="G$1" pin="RESETB" pad="21"/>
<connect gate="G$1" pin="SDATA0" pad="15"/>
<connect gate="G$1" pin="SDATA1" pad="11"/>
<connect gate="G$1" pin="SDATA2" pad="8"/>
<connect gate="G$1" pin="SDATAOUT" pad="41"/>
<connect gate="G$1" pin="VOUTL+" pad="33"/>
<connect gate="G$1" pin="VOUTL-" pad="34"/>
<connect gate="G$1" pin="VOUTR+" pad="29"/>
<connect gate="G$1" pin="VOUTR-" pad="28"/>
<connect gate="G$1" pin="VOUTS+" pad="26"/>
<connect gate="G$1" pin="VOUTS-" pad="25"/>
<connect gate="G$1" pin="VREF" pad="38"/>
<connect gate="G$1" pin="ZEROFLAG" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD1954YSTZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12M8458"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1983" prefix="IC">
<description>&lt;b&gt;HD Audio SoundMAX® Codec&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1983.pdf</description>
<gates>
<gate name="G$1" symbol="AD1983"/>
</gates>
<devices>
<device name="" package="LFCSP32">
<connects>
<connect gate="G$1" pin="AVDD" pad="22"/>
<connect gate="G$1" pin="AVDD@1" pad="26"/>
<connect gate="G$1" pin="AVSS" pad="17"/>
<connect gate="G$1" pin="AVSS@1" pad="29"/>
<connect gate="G$1" pin="BIT_CLK" pad="3"/>
<connect gate="G$1" pin="DVDD" pad="6"/>
<connect gate="G$1" pin="DVSS" pad="4"/>
<connect gate="G$1" pin="GPIO_0/JS_1" pad="30"/>
<connect gate="G$1" pin="GPIO_1/JS_0" pad="31"/>
<connect gate="G$1" pin="MIC_BIAS-B" pad="19"/>
<connect gate="G$1" pin="MIC_BIAS-C" pad="20"/>
<connect gate="G$1" pin="MONO_OUT" pad="25"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="10"/>
<connect gate="G$1" pin="NC@2" pad="11"/>
<connect gate="G$1" pin="NC@3" pad="12"/>
<connect gate="G$1" pin="PORT-A_L" pad="27"/>
<connect gate="G$1" pin="PORT-A_R" pad="28"/>
<connect gate="G$1" pin="PORT-B_L" pad="13"/>
<connect gate="G$1" pin="PORT-B_R" pad="14"/>
<connect gate="G$1" pin="PORT-C_L" pad="15"/>
<connect gate="G$1" pin="PORT-C_R" pad="16"/>
<connect gate="G$1" pin="PORT-D_L" pad="23"/>
<connect gate="G$1" pin="PORT-D_R" pad="24"/>
<connect gate="G$1" pin="RESET" pad="8"/>
<connect gate="G$1" pin="S/PDIF_OUT" pad="32"/>
<connect gate="G$1" pin="SDATA_IN" pad="5"/>
<connect gate="G$1" pin="SDATA_OUT" pad="2"/>
<connect gate="G$1" pin="SENSE_A" pad="9"/>
<connect gate="G$1" pin="SENSE_SRC" pad="21"/>
<connect gate="G$1" pin="SYNC" pad="7"/>
<connect gate="G$1" pin="VREF_FILT" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD1985" prefix="IC">
<description>&lt;b&gt;AC ?97 SoundMAX® Codec&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD1985.pdf</description>
<gates>
<gate name="G$1" symbol="AD1985"/>
</gates>
<devices>
<device name="" package="QFP-7X7-48">
<connects>
<connect gate="G$1" pin="AFILT1" pad="29"/>
<connect gate="G$1" pin="AFLIT2" pad="30"/>
<connect gate="G$1" pin="AUX_L" pad="14"/>
<connect gate="G$1" pin="AUX_R" pad="15"/>
<connect gate="G$1" pin="AVDD1" pad="25"/>
<connect gate="G$1" pin="AVDD2" pad="38"/>
<connect gate="G$1" pin="AVDD3" pad="43"/>
<connect gate="G$1" pin="AVDD4" pad="34"/>
<connect gate="G$1" pin="AVSS1" pad="26"/>
<connect gate="G$1" pin="AVSS2" pad="40"/>
<connect gate="G$1" pin="AVSS3" pad="44"/>
<connect gate="G$1" pin="BIT_CLK" pad="6"/>
<connect gate="G$1" pin="CD_GND_REF" pad="19"/>
<connect gate="G$1" pin="CD_L" pad="18"/>
<connect gate="G$1" pin="CD_R" pad="20"/>
<connect gate="G$1" pin="CENTER_OUT" pad="31"/>
<connect gate="G$1" pin="DVDD1" pad="1"/>
<connect gate="G$1" pin="DVDD2" pad="9"/>
<connect gate="G$1" pin="DVSS1" pad="4"/>
<connect gate="G$1" pin="DVSS2" pad="7"/>
<connect gate="G$1" pin="EAPD" pad="47"/>
<connect gate="G$1" pin="ID0" pad="45"/>
<connect gate="G$1" pin="ID1" pad="46"/>
<connect gate="G$1" pin="JS0" pad="17"/>
<connect gate="G$1" pin="JS1" pad="16"/>
<connect gate="G$1" pin="JS2" pad="33"/>
<connect gate="G$1" pin="JS3" pad="12"/>
<connect gate="G$1" pin="LFE_OUT" pad="32"/>
<connect gate="G$1" pin="LINE_IN_L" pad="23"/>
<connect gate="G$1" pin="LINE_IN_R" pad="24"/>
<connect gate="G$1" pin="LINE_OUT_L/SURR_L" pad="35"/>
<connect gate="G$1" pin="LINE_OUT_R/SURR_R" pad="36"/>
<connect gate="G$1" pin="MIC1" pad="21"/>
<connect gate="G$1" pin="MIC2" pad="22"/>
<connect gate="G$1" pin="MONO_OUT" pad="37"/>
<connect gate="G$1" pin="NC" pad="42"/>
<connect gate="G$1" pin="PHONE_IN" pad="13"/>
<connect gate="G$1" pin="RESET" pad="11"/>
<connect gate="G$1" pin="SDATA_IN" pad="8"/>
<connect gate="G$1" pin="SDATA_OUT" pad="5"/>
<connect gate="G$1" pin="SPDIF" pad="48"/>
<connect gate="G$1" pin="SURR_OUT_L/HP_OUT_L" pad="39"/>
<connect gate="G$1" pin="SURR_OUT_R/HP_OUT_R" pad="41"/>
<connect gate="G$1" pin="SYNC" pad="10"/>
<connect gate="G$1" pin="VREF" pad="27"/>
<connect gate="G$1" pin="VREFOUT" pad="28"/>
<connect gate="G$1" pin="XTL_IN" pad="2"/>
<connect gate="G$1" pin="XTL_OUT" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD210" prefix="IC">
<description>&lt;b&gt;Precision, Wide Bandwidth 3-Port Isolation Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD210.pdf</description>
<gates>
<gate name="G$1" symbol="AD210"/>
</gates>
<devices>
<device name="" package="AD210">
<connects>
<connect gate="G$1" pin="+IN" pad="19"/>
<connect gate="G$1" pin="+VISS" pad="14"/>
<connect gate="G$1" pin="+VOSS" pad="3"/>
<connect gate="G$1" pin="-IN" pad="17"/>
<connect gate="G$1" pin="-VISS" pad="15"/>
<connect gate="G$1" pin="-VOSS" pad="4"/>
<connect gate="G$1" pin="FB" pad="16"/>
<connect gate="G$1" pin="ICOM" pad="18"/>
<connect gate="G$1" pin="OCOM" pad="2"/>
<connect gate="G$1" pin="PWR" pad="30"/>
<connect gate="G$1" pin="PWR_COM" pad="29"/>
<connect gate="G$1" pin="VO" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD210AN"/>
<attribute name="OC_FARNELL" value="3182034"/>
<attribute name="OC_NEWARK" value="05F6727"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD215" prefix="IC">
<description>&lt;b&gt;120 kHz Bandwidth, Low Distortion, Isolation Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD215.pdf</description>
<gates>
<gate name="G$1" symbol="AD215"/>
</gates>
<devices>
<device name="" package="AD215">
<connects>
<connect gate="G$1" pin="+15V" pad="42"/>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+VISO" pad="6"/>
<connect gate="G$1" pin="-15V" pad="44"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="-VISO" pad="5"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="INCOM" pad="2"/>
<connect gate="G$1" pin="OUTHI" pad="38"/>
<connect gate="G$1" pin="OUTLO" pad="37"/>
<connect gate="G$1" pin="PWRRTN" pad="43"/>
<connect gate="G$1" pin="TRIM" pad="36"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD215AY"/>
<attribute name="OC_FARNELL" value="1464281"/>
<attribute name="OC_NEWARK" value="09B5050"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD526" prefix="IC">
<description>&lt;b&gt;Monolithic Software Programmable Gain Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.dscc.dla.mil/Downloads/MilSpec/Smd/90894.pdf</description>
<gates>
<gate name="G$1" symbol="AD526"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="!CLK" pad="13"/>
<connect gate="G$1" pin="!CS" pad="14"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="12"/>
<connect gate="G$1" pin="AGND1" pad="6"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="B" pad="11"/>
<connect gate="G$1" pin="DGND" pad="1"/>
<connect gate="G$1" pin="NULL@1" pad="2"/>
<connect gate="G$1" pin="NULL@2" pad="4"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VO/F" pad="9"/>
<connect gate="G$1" pin="VO/S" pad="8"/>
<connect gate="G$1" pin="VS+" pad="10"/>
<connect gate="G$1" pin="VS-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD526AD"/>
<attribute name="OC_FARNELL" value="402140"/>
<attribute name="OC_NEWARK" value="05F6913"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD623" prefix="IC">
<description>&lt;b&gt;Single-Supply, Rail-to-Rail, Low Cost Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD623.pdf</description>
<gates>
<gate name="G$1" symbol="AD620"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="+V" pad="7"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="1"/>
<connect gate="G$1" pin="RG@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD623ANZ"/>
<attribute name="OC_FARNELL" value="9603700"/>
<attribute name="OC_NEWARK" value="59K4402"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="+V" pad="7"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="1"/>
<connect gate="G$1" pin="RG@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD623ARZ."/>
<attribute name="OC_FARNELL" value="9426213"/>
<attribute name="OC_NEWARK" value="31M4186"/>
</technology>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="+V" pad="7"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="1"/>
<connect gate="G$1" pin="RG@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD623ARMZ"/>
<attribute name="OC_FARNELL" value="1660961"/>
<attribute name="OC_NEWARK" value="19M8824"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD625" prefix="IC">
<description>&lt;b&gt;Programmable Gain Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD625.pdf</description>
<gates>
<gate name="G$1" symbol="AD625"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="+GAINDRIVE" pad="12"/>
<connect gate="G$1" pin="+GAINSENSE" pad="2"/>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+VS" pad="9"/>
<connect gate="G$1" pin="-GAINDRIVE" pad="5"/>
<connect gate="G$1" pin="-GAINSENSE" pad="15"/>
<connect gate="G$1" pin="-IN" pad="16"/>
<connect gate="G$1" pin="-VS" pad="8"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="RTINULL@1" pad="3"/>
<connect gate="G$1" pin="RTINULL@2" pad="4"/>
<connect gate="G$1" pin="RTONULL@1" pad="14"/>
<connect gate="G$1" pin="RTONULL@2" pad="13"/>
<connect gate="G$1" pin="SENSE" pad="11"/>
<connect gate="G$1" pin="VOUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD625KNZ"/>
<attribute name="OC_FARNELL" value="1438353"/>
<attribute name="OC_NEWARK" value="15P0739"/>
</technology>
</technologies>
</device>
<device name="D" package="DIL16">
<connects>
<connect gate="G$1" pin="+GAINDRIVE" pad="12"/>
<connect gate="G$1" pin="+GAINSENSE" pad="2"/>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+VS" pad="9"/>
<connect gate="G$1" pin="-GAINDRIVE" pad="5"/>
<connect gate="G$1" pin="-GAINSENSE" pad="15"/>
<connect gate="G$1" pin="-IN" pad="16"/>
<connect gate="G$1" pin="-VS" pad="8"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="RTINULL@1" pad="3"/>
<connect gate="G$1" pin="RTINULL@2" pad="4"/>
<connect gate="G$1" pin="RTONULL@1" pad="14"/>
<connect gate="G$1" pin="RTONULL@2" pad="13"/>
<connect gate="G$1" pin="SENSE" pad="11"/>
<connect gate="G$1" pin="VOUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD625KNZ"/>
<attribute name="OC_FARNELL" value="3182289"/>
<attribute name="OC_NEWARK" value="15P0739"/>
</technology>
</technologies>
</device>
<device name="E" package="PLCC20">
<connects>
<connect gate="G$1" pin="+GAINDRIVE" pad="7"/>
<connect gate="G$1" pin="+GAINSENSE" pad="3"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VS" pad="12"/>
<connect gate="G$1" pin="-GAINDRIVE" pad="15"/>
<connect gate="G$1" pin="-GAINSENSE" pad="19"/>
<connect gate="G$1" pin="-IN" pad="20"/>
<connect gate="G$1" pin="-VS" pad="10"/>
<connect gate="G$1" pin="REF" pad="9"/>
<connect gate="G$1" pin="RTINULL@1" pad="4"/>
<connect gate="G$1" pin="RTINULL@2" pad="5"/>
<connect gate="G$1" pin="RTONULL@1" pad="18"/>
<connect gate="G$1" pin="RTONULL@2" pad="17"/>
<connect gate="G$1" pin="SENSE" pad="14"/>
<connect gate="G$1" pin="VOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD627" prefix="IC">
<description>&lt;b&gt;Micropower, Single- and Dual-Supply, Rail-to-Rail Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD627.pdf</description>
<gates>
<gate name="G$1" symbol="AD620"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="+V" pad="7"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="1"/>
<connect gate="G$1" pin="RG@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD627BNZ"/>
<attribute name="OC_FARNELL" value="1438354"/>
<attribute name="OC_NEWARK" value="59K4418"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="+V" pad="7"/>
<connect gate="G$1" pin="-" pad="2"/>
<connect gate="G$1" pin="-V" pad="4"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="1"/>
<connect gate="G$1" pin="RG@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD627AR"/>
<attribute name="OC_FARNELL" value="1438354"/>
<attribute name="OC_NEWARK" value="09B5402"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD711" prefix="IC">
<description>&lt;b&gt;Precision, Low Cost, High Speed, BiFET Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD711.pdf</description>
<gates>
<gate name="G$1" symbol="OP_OFFSET+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD711BQ"/>
<attribute name="OC_FARNELL" value="9604839"/>
<attribute name="OC_NEWARK" value="66F5826"/>
</technology>
</technologies>
</device>
<device name="RN" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD711KRZ"/>
<attribute name="OC_FARNELL" value="9426396"/>
<attribute name="OC_NEWARK" value="59K4541"/>
</technology>
</technologies>
</device>
<device name="H" package="H08">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD712" prefix="IC">
<description>&lt;b&gt;Dual Precision, Low Cost, High Speed BiFET Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD712.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD712JNZ"/>
<attribute name="OC_FARNELL" value="9604898"/>
<attribute name="OC_NEWARK" value="59K4554"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD712KRZ"/>
<attribute name="OC_FARNELL" value="1263975"/>
<attribute name="OC_NEWARK" value="59K4556"/>
</technology>
</technologies>
</device>
<device name="Q" package="DIL08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD712AQ"/>
<attribute name="OC_FARNELL" value="9604898"/>
<attribute name="OC_NEWARK" value="05F7274"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD744" prefix="IC">
<description>&lt;b&gt;Precision, 500 ns Settling BiFET Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD744.pdf</description>
<gates>
<gate name="P" symbol="OP-COMP+-VS"/>
</gates>
<devices>
<device name="H" package="H08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="COMP" pad="5"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="COMP" pad="5"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD744JNZ"/>
<attribute name="OC_FARNELL" value="1438362"/>
<attribute name="OC_NEWARK" value="59K4810"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="COMP" pad="5"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ANALOG DEVICES"/>
<attribute name="MPN" value="AD744JR"/>
<attribute name="OC_FARNELL" value="1651300"/>
<attribute name="OC_NEWARK" value="05F7341"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD745" prefix="IC">
<description>&lt;b&gt;Ultralow Noise, High Speed, BiFET Op Amp&lt;/b&gt;&lt;p&gt;
Course: http://www.analog.com/static/imported-files/data_sheets/AD745.pdf</description>
<gates>
<gate name="P" symbol="OP_OFFSET+-VS"/>
</gates>
<devices>
<device name="R" package="SOIC16R">
<connects>
<connect gate="P" pin="+VS" pad="13"/>
<connect gate="P" pin="-VS" pad="6"/>
<connect gate="P" pin="IN+" pad="5"/>
<connect gate="P" pin="IN-" pad="3"/>
<connect gate="P" pin="OFF@1" pad="2"/>
<connect gate="P" pin="OFF@2" pad="11"/>
<connect gate="P" pin="OUT" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD745JRZ-16"/>
<attribute name="OC_FARNELL" value="1838876"/>
<attribute name="OC_NEWARK" value="59K4819"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD746" prefix="IC">
<description>&lt;b&gt;Dual Precision, 500 ns Settling, BiFET Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD746.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD746JNZ"/>
<attribute name="OC_FARNELL" value="1438363"/>
<attribute name="OC_NEWARK" value="59K4844"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD746JRZ"/>
<attribute name="OC_FARNELL" value="1423876"/>
<attribute name="OC_NEWARK" value="59K4845"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7676" prefix="IC">
<description>&lt;b&gt;16-Bit, +-1 LSB INL, 500 kSPS, Differential ADC&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD7676.pdf</description>
<gates>
<gate name="G$" symbol="AD7676"/>
</gates>
<devices>
<device name="CP" package="LFCSP48">
<connects>
<connect gate="G$" pin="!CNVST" pad="35"/>
<connect gate="G$" pin="!CS" pad="32"/>
<connect gate="G$" pin="!RD" pad="31"/>
<connect gate="G$" pin="AGND@1" pad="1"/>
<connect gate="G$" pin="AGND@2" pad="36"/>
<connect gate="G$" pin="AVDD" pad="2"/>
<connect gate="G$" pin="BUSY" pad="29"/>
<connect gate="G$" pin="BYTESWAP" pad="4"/>
<connect gate="G$" pin="D0" pad="9"/>
<connect gate="G$" pin="D1" pad="10"/>
<connect gate="G$" pin="D12" pad="25"/>
<connect gate="G$" pin="D13" pad="26"/>
<connect gate="G$" pin="D14" pad="27"/>
<connect gate="G$" pin="D15" pad="28"/>
<connect gate="G$" pin="DGND@1" pad="20"/>
<connect gate="G$" pin="DGND@2" pad="30"/>
<connect gate="G$" pin="DIVSCLK0/D2" pad="11"/>
<connect gate="G$" pin="DIVSCLK1/D3" pad="12"/>
<connect gate="G$" pin="DVDD" pad="19"/>
<connect gate="G$" pin="EXT/!INT!/D4" pad="13"/>
<connect gate="G$" pin="IN+" pad="43"/>
<connect gate="G$" pin="IN-" pad="39"/>
<connect gate="G$" pin="INVSCLK/D6" pad="15"/>
<connect gate="G$" pin="INVSYNC/D5" pad="14"/>
<connect gate="G$" pin="OB/!2C" pad="5"/>
<connect gate="G$" pin="OGND" pad="17"/>
<connect gate="G$" pin="OVDD" pad="18"/>
<connect gate="G$" pin="PD" pad="34"/>
<connect gate="G$" pin="RDC/SDIN/D7" pad="16"/>
<connect gate="G$" pin="RDERROR/D11" pad="24"/>
<connect gate="G$" pin="REF" pad="37"/>
<connect gate="G$" pin="REFGND" pad="38"/>
<connect gate="G$" pin="RESET" pad="33"/>
<connect gate="G$" pin="SCLK/D9" pad="22"/>
<connect gate="G$" pin="SDOUT/D8" pad="21"/>
<connect gate="G$" pin="SER/!PAR" pad="8"/>
<connect gate="G$" pin="SYNC/D10" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7676ASTZ"/>
<attribute name="OC_FARNELL" value="1464604"/>
<attribute name="OC_NEWARK" value="59K5190"/>
</technology>
</technologies>
</device>
<device name="ST" package="QFP-7X7-48">
<connects>
<connect gate="G$" pin="!CNVST" pad="35"/>
<connect gate="G$" pin="!CS" pad="32"/>
<connect gate="G$" pin="!RD" pad="31"/>
<connect gate="G$" pin="AGND@1" pad="1"/>
<connect gate="G$" pin="AGND@2" pad="36"/>
<connect gate="G$" pin="AVDD" pad="2"/>
<connect gate="G$" pin="BUSY" pad="29"/>
<connect gate="G$" pin="BYTESWAP" pad="4"/>
<connect gate="G$" pin="D0" pad="9"/>
<connect gate="G$" pin="D1" pad="10"/>
<connect gate="G$" pin="D12" pad="25"/>
<connect gate="G$" pin="D13" pad="26"/>
<connect gate="G$" pin="D14" pad="27"/>
<connect gate="G$" pin="D15" pad="28"/>
<connect gate="G$" pin="DGND@1" pad="20"/>
<connect gate="G$" pin="DGND@2" pad="30"/>
<connect gate="G$" pin="DIVSCLK0/D2" pad="11"/>
<connect gate="G$" pin="DIVSCLK1/D3" pad="12"/>
<connect gate="G$" pin="DVDD" pad="19"/>
<connect gate="G$" pin="EXT/!INT!/D4" pad="13"/>
<connect gate="G$" pin="IN+" pad="43"/>
<connect gate="G$" pin="IN-" pad="39"/>
<connect gate="G$" pin="INVSCLK/D6" pad="15"/>
<connect gate="G$" pin="INVSYNC/D5" pad="14"/>
<connect gate="G$" pin="OB/!2C" pad="5"/>
<connect gate="G$" pin="OGND" pad="17"/>
<connect gate="G$" pin="OVDD" pad="18"/>
<connect gate="G$" pin="PD" pad="34"/>
<connect gate="G$" pin="RDC/SDIN/D7" pad="16"/>
<connect gate="G$" pin="RDERROR/D11" pad="24"/>
<connect gate="G$" pin="REF" pad="37"/>
<connect gate="G$" pin="REFGND" pad="38"/>
<connect gate="G$" pin="RESET" pad="33"/>
<connect gate="G$" pin="SCLK/D9" pad="22"/>
<connect gate="G$" pin="SDOUT/D8" pad="21"/>
<connect gate="G$" pin="SER/!PAR" pad="8"/>
<connect gate="G$" pin="SYNC/D10" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7676ASTZRL"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K5191"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD7730" prefix="IC">
<description>&lt;b&gt;Bridge Transducer ADC&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD7730_7730L.pdf</description>
<gates>
<gate name="P" symbol="AD7730"/>
</gates>
<devices>
<device name="R" package="SO24R">
<connects>
<connect gate="P" pin="!ACX" pad="17"/>
<connect gate="P" pin="!CS" pad="19"/>
<connect gate="P" pin="!RDY" pad="20"/>
<connect gate="P" pin="!RESET" pad="6"/>
<connect gate="P" pin="!STANDBY" pad="18"/>
<connect gate="P" pin="!SYNC" pad="5"/>
<connect gate="P" pin="ACX" pad="16"/>
<connect gate="P" pin="AGND" pad="8"/>
<connect gate="P" pin="AIN1+" pad="10"/>
<connect gate="P" pin="AIN1-" pad="11"/>
<connect gate="P" pin="AIN2+/D1" pad="12"/>
<connect gate="P" pin="AIN2-/D0" pad="13"/>
<connect gate="P" pin="AVDD" pad="9"/>
<connect gate="P" pin="DGND" pad="24"/>
<connect gate="P" pin="DIN" pad="22"/>
<connect gate="P" pin="DOUT" pad="21"/>
<connect gate="P" pin="DVDD" pad="23"/>
<connect gate="P" pin="MCLKIN" pad="2"/>
<connect gate="P" pin="MCLKOUT" pad="3"/>
<connect gate="P" pin="POL" pad="4"/>
<connect gate="P" pin="REFIN+" pad="14"/>
<connect gate="P" pin="REFIN-" pad="15"/>
<connect gate="P" pin="SCLK" pad="1"/>
<connect gate="P" pin="VBIAS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7730LBRZ"/>
<attribute name="OC_FARNELL" value="1079295"/>
<attribute name="OC_NEWARK" value="59K5383"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP24">
<connects>
<connect gate="P" pin="!ACX" pad="17"/>
<connect gate="P" pin="!CS" pad="19"/>
<connect gate="P" pin="!RDY" pad="20"/>
<connect gate="P" pin="!RESET" pad="6"/>
<connect gate="P" pin="!STANDBY" pad="18"/>
<connect gate="P" pin="!SYNC" pad="5"/>
<connect gate="P" pin="ACX" pad="16"/>
<connect gate="P" pin="AGND" pad="8"/>
<connect gate="P" pin="AIN1+" pad="10"/>
<connect gate="P" pin="AIN1-" pad="11"/>
<connect gate="P" pin="AIN2+/D1" pad="12"/>
<connect gate="P" pin="AIN2-/D0" pad="13"/>
<connect gate="P" pin="AVDD" pad="9"/>
<connect gate="P" pin="DGND" pad="24"/>
<connect gate="P" pin="DIN" pad="22"/>
<connect gate="P" pin="DOUT" pad="21"/>
<connect gate="P" pin="DVDD" pad="23"/>
<connect gate="P" pin="MCLKIN" pad="2"/>
<connect gate="P" pin="MCLKOUT" pad="3"/>
<connect gate="P" pin="POL" pad="4"/>
<connect gate="P" pin="REFIN+" pad="14"/>
<connect gate="P" pin="REFIN-" pad="15"/>
<connect gate="P" pin="SCLK" pad="1"/>
<connect gate="P" pin="VBIAS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7730BRUZ"/>
<attribute name="OC_FARNELL" value="1423932"/>
<attribute name="OC_NEWARK" value="59K5374"/>
</technology>
</technologies>
</device>
<device name="N" package="DIL24-3">
<connects>
<connect gate="P" pin="!ACX" pad="17"/>
<connect gate="P" pin="!CS" pad="19"/>
<connect gate="P" pin="!RDY" pad="20"/>
<connect gate="P" pin="!RESET" pad="6"/>
<connect gate="P" pin="!STANDBY" pad="18"/>
<connect gate="P" pin="!SYNC" pad="5"/>
<connect gate="P" pin="ACX" pad="16"/>
<connect gate="P" pin="AGND" pad="8"/>
<connect gate="P" pin="AIN1+" pad="10"/>
<connect gate="P" pin="AIN1-" pad="11"/>
<connect gate="P" pin="AIN2+/D1" pad="12"/>
<connect gate="P" pin="AIN2-/D0" pad="13"/>
<connect gate="P" pin="AVDD" pad="9"/>
<connect gate="P" pin="DGND" pad="24"/>
<connect gate="P" pin="DIN" pad="22"/>
<connect gate="P" pin="DOUT" pad="21"/>
<connect gate="P" pin="DVDD" pad="23"/>
<connect gate="P" pin="MCLKIN" pad="2"/>
<connect gate="P" pin="MCLKOUT" pad="3"/>
<connect gate="P" pin="POL" pad="4"/>
<connect gate="P" pin="REFIN+" pad="14"/>
<connect gate="P" pin="REFIN-" pad="15"/>
<connect gate="P" pin="SCLK" pad="1"/>
<connect gate="P" pin="VBIAS" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD7730BN"/>
<attribute name="OC_FARNELL" value="9605487"/>
<attribute name="OC_NEWARK" value="48F1987"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD797" prefix="IC">
<description>&lt;b&gt;Ultralow Distortion, Ultralow Noise Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD797.pdf</description>
<gates>
<gate name="P" symbol="OP-COMP+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="COMP" pad="8"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="5"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD797ANZ"/>
<attribute name="OC_FARNELL" value="9603778"/>
<attribute name="OC_NEWARK" value="59K6088"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="COMP" pad="8"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="5"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD797ARZ"/>
<attribute name="OC_FARNELL" value="9426450"/>
<attribute name="OC_NEWARK" value="88H0085"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8001" prefix="IC">
<description>&lt;b&gt;800 MHz, 50 mW Current Feedback Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8001.pdf</description>
<gates>
<gate name="P" symbol="OP+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8001ANZ"/>
<attribute name="OC_FARNELL" value="9605304"/>
<attribute name="OC_NEWARK" value="19M0911"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8001AR"/>
<attribute name="OC_FARNELL" value="9605657"/>
<attribute name="OC_NEWARK" value="05F7664"/>
</technology>
</technologies>
</device>
<device name="RT" package="SOT23-5">
<connects>
<connect gate="P" pin="+VS" pad="5"/>
<connect gate="P" pin="-VS" pad="2"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="4"/>
<connect gate="P" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8001ARTZ-REEL7"/>
<attribute name="OC_FARNELL" value="1651271"/>
<attribute name="OC_NEWARK" value="59K6136"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8015" prefix="IC">
<description>&lt;b&gt;Wideband/Differential Output Transimpedance Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8015.pdf</description>
<gates>
<gate name="P" symbol="AD8015"/>
</gates>
<devices>
<device name="" package="SO8">
<connects>
<connect gate="P" pin="+OUT" pad="7"/>
<connect gate="P" pin="+VS" pad="8"/>
<connect gate="P" pin="-OUT" pad="6"/>
<connect gate="P" pin="-VS" pad="5"/>
<connect gate="P" pin="IN" pad="2"/>
<connect gate="P" pin="VBYP" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8015ARZ"/>
<attribute name="OC_FARNELL" value="1464812"/>
<attribute name="OC_NEWARK" value="19M8870"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8031" prefix="IC">
<description>&lt;b&gt;2.7 V, 800 ?A, 80 MHz Rail-to-Rail I/O Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8031_8032.pdf</description>
<gates>
<gate name="P" symbol="OP+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8031BNZ"/>
<attribute name="OC_FARNELL" value="1438575"/>
<attribute name="OC_NEWARK" value="15P0920"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8031ARZ"/>
<attribute name="OC_FARNELL" value="8621500"/>
<attribute name="OC_NEWARK" value="19M0917"/>
</technology>
</technologies>
</device>
<device name="RJ" package="SOT23-5">
<connects>
<connect gate="P" pin="+VS" pad="5"/>
<connect gate="P" pin="-VS" pad="2"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="4"/>
<connect gate="P" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8031ARTZ-REEL7"/>
<attribute name="OC_FARNELL" value="1660972"/>
<attribute name="OC_NEWARK" value="84R8399"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8033" prefix="IC">
<description>&lt;b&gt;2.7 V, 800 ?A, 80 MHz Rail-to-Rail I/O Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8031_8032.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8033ARZ"/>
<attribute name="OC_FARNELL" value="8621519"/>
<attribute name="OC_NEWARK" value="59K6245"/>
</technology>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8033ARZ-REEL"/>
<attribute name="OC_FARNELL" value="8621519"/>
<attribute name="OC_NEWARK" value="59K6246"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8041" prefix="IC">
<description>&lt;b&gt;160 MHz Rail-to-Rail Amplifier with Disable&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8041.pdf</description>
<gates>
<gate name="P" symbol="OP+-VSDISABLE"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="DISABLE" pad="8"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8041ANZ"/>
<attribute name="OC_FARNELL" value="1438577"/>
<attribute name="OC_NEWARK" value="15P0923"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="DISABLE" pad="8"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8041ARZ"/>
<attribute name="OC_FARNELL" value="1464831"/>
<attribute name="OC_NEWARK" value="88H0130"/>
</technology>
</technologies>
</device>
<device name="Q" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="DISABLE" pad="8"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8041ANZ"/>
<attribute name="OC_FARNELL" value="1438577"/>
<attribute name="OC_NEWARK" value="15P0923"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8042" prefix="IC">
<description>&lt;b&gt;Dual 160 MHz Rail-to-Rail Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8042.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ANALOG DEVICES"/>
<attribute name="MPN" value="AD8042AN"/>
<attribute name="OC_FARNELL" value="1540543"/>
<attribute name="OC_NEWARK" value="52F8033"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8042AR"/>
<attribute name="OC_FARNELL" value="1424032"/>
<attribute name="OC_NEWARK" value="52F8034"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8065" prefix="IC">
<description>&lt;b&gt;High Performance, 145 MHz FastFET Op Amps&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8065_8066.pdf</description>
<gates>
<gate name="G$" symbol="OP+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$" pin="+VS" pad="7"/>
<connect gate="G$" pin="-VS" pad="4"/>
<connect gate="G$" pin="IN+" pad="3"/>
<connect gate="G$" pin="IN-" pad="2"/>
<connect gate="G$" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="G$" pin="+VS" pad="7"/>
<connect gate="G$" pin="-VS" pad="4"/>
<connect gate="G$" pin="IN+" pad="3"/>
<connect gate="G$" pin="IN-" pad="2"/>
<connect gate="G$" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="RT" package="SOT23-5">
<connects>
<connect gate="G$" pin="+VS" pad="5"/>
<connect gate="G$" pin="-VS" pad="2"/>
<connect gate="G$" pin="IN+" pad="3"/>
<connect gate="G$" pin="IN-" pad="4"/>
<connect gate="G$" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8065ARTZ-REEL7"/>
<attribute name="OC_FARNELL" value="1464845"/>
<attribute name="OC_NEWARK" value="59K6316"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8066" prefix="IC">
<description>&lt;b&gt;High Performance, 145 MHz FastFET Op Amps&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8065_8066.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD807*" prefix="IC">
<description>&lt;b&gt;500 MHz, G = +1 and +2 Triple Video Buffers with Disable&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8074_8075.pdf</description>
<gates>
<gate name="P" symbol="AD8074"/>
</gates>
<devices>
<device name="RU" package="TSSOP16">
<connects>
<connect gate="P" pin="!OE" pad="1"/>
<connect gate="P" pin="AGND@1" pad="4"/>
<connect gate="P" pin="AGND@2" pad="6"/>
<connect gate="P" pin="DGND" pad="2"/>
<connect gate="P" pin="IN0" pad="7"/>
<connect gate="P" pin="IN1" pad="5"/>
<connect gate="P" pin="IN2" pad="3"/>
<connect gate="P" pin="OUT0" pad="10"/>
<connect gate="P" pin="OUT1" pad="12"/>
<connect gate="P" pin="OUT2" pad="14"/>
<connect gate="P" pin="VCC@1" pad="11"/>
<connect gate="P" pin="VCC@2" pad="15"/>
<connect gate="P" pin="VCC@3" pad="16"/>
<connect gate="P" pin="VEE@1" pad="8"/>
<connect gate="P" pin="VEE@2" pad="9"/>
<connect gate="P" pin="VEE@3" pad="13"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8074ARUZ"/>
<attribute name="OC_FARNELL" value="9426027"/>
<attribute name="OC_NEWARK" value="19M0929"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8075ARUZ"/>
<attribute name="OC_FARNELL" value="9426035"/>
<attribute name="OC_NEWARK" value="19M0930"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8079" prefix="IC">
<description>&lt;b&gt;Dual 260 MHz Gain = +2.0 &amp; +2.2 Buffer&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8079.pdf</description>
<gates>
<gate name="A" symbol="OP-GAIN"/>
<gate name="B" symbol="OP-GAIN"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="" package="SO8">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN+" pad="1"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="B" pin="GND" pad="3"/>
<connect gate="B" pin="IN+" pad="4"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8079BRZ"/>
<attribute name="OC_FARNELL" value="1838858"/>
<attribute name="OC_NEWARK" value="59K6340"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD811" prefix="IC">
<description>&lt;b&gt;High Performance Video Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD811.pdf</description>
<gates>
<gate name="G$" symbol="OP+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$" pin="+VS" pad="7"/>
<connect gate="G$" pin="-VS" pad="4"/>
<connect gate="G$" pin="IN+" pad="3"/>
<connect gate="G$" pin="IN-" pad="2"/>
<connect gate="G$" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD811AN"/>
<attribute name="OC_FARNELL" value="1464857"/>
<attribute name="OC_NEWARK" value="05F7667"/>
</technology>
</technologies>
</device>
<device name="R-8" package="SO8">
<connects>
<connect gate="G$" pin="+VS" pad="7"/>
<connect gate="G$" pin="-VS" pad="4"/>
<connect gate="G$" pin="IN+" pad="3"/>
<connect gate="G$" pin="IN-" pad="2"/>
<connect gate="G$" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD811JRZ"/>
<attribute name="OC_FARNELL" value="9426485"/>
<attribute name="OC_NEWARK" value="82H2980"/>
</technology>
</technologies>
</device>
<device name="R-16" package="SOIC16R">
<connects>
<connect gate="G$" pin="+VS" pad="14"/>
<connect gate="G$" pin="-VS" pad="7"/>
<connect gate="G$" pin="IN+" pad="5"/>
<connect gate="G$" pin="IN-" pad="3"/>
<connect gate="G$" pin="OUT" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD811ARZ-16"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K6371"/>
</technology>
</technologies>
</device>
<device name="E" package="PLCC20">
<connects>
<connect gate="G$" pin="+VS" pad="16"/>
<connect gate="G$" pin="-VS" pad="9"/>
<connect gate="G$" pin="IN+" pad="8"/>
<connect gate="G$" pin="IN-" pad="6"/>
<connect gate="G$" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R-20" package="SOIC20R">
<connects>
<connect gate="G$" pin="+VS" pad="17"/>
<connect gate="G$" pin="-VS" pad="8"/>
<connect gate="G$" pin="IN+" pad="6"/>
<connect gate="G$" pin="IN-" pad="4"/>
<connect gate="G$" pin="OUT" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD811ARZ-20"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K6374"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD817" prefix="IC">
<description>&lt;b&gt;High Speed, Low Power Wide Supply Range Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD817.pdf</description>
<gates>
<gate name="P" symbol="OP_OFFSET+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="9604006"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD817ARZ"/>
<attribute name="OC_FARNELL" value="1660992"/>
<attribute name="OC_NEWARK" value="88H0179"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD818" prefix="IC">
<description>&lt;b&gt;Low Cost, Low Power Video Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD818.pdf</description>
<gates>
<gate name="P" symbol="OP_OFFSET+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="9605630"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD818ARZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="82H2988"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD820N" prefix="IC">
<description>&lt;b&gt;Single-Supply, Rail-to-Rail, Low Power, FET Input Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD820.pdf</description>
<gates>
<gate name="G$1" symbol="OP_OFFSET+-VS"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1438579"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD820" prefix="IC">
<description>&lt;b&gt;Single-Supply, Rail-to-Rail, Low Power, FET Input Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD820.pdf</description>
<gates>
<gate name="G$1" symbol="OP+-VS"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1838867"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD820ARZ"/>
<attribute name="OC_FARNELL" value="9426469"/>
<attribute name="OC_NEWARK" value="88H0196"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD822" prefix="IC">
<description>&lt;b&gt;Single-Supply, Rail-to-Rail Low Power FET-Input Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD822.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1438581"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ANALOG DEVICES"/>
<attribute name="MPN" value="AD822BRZ"/>
<attribute name="OC_FARNELL" value="1651303"/>
</technology>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD822ARMZ-R2"/>
<attribute name="OC_FARNELL" value="1827360"/>
<attribute name="OC_NEWARK" value="19M8890"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD825" prefix="IC">
<description>&lt;b&gt;Low Cost, General-Purpose High Speed JFET Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD825.pdf</description>
<gates>
<gate name="P" symbol="OP+-VS"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD825ARZ"/>
<attribute name="OC_FARNELL" value="9603735"/>
<attribute name="OC_NEWARK" value="59K6528"/>
</technology>
</technologies>
</device>
<device name="R-16" package="SOIC16R">
<connects>
<connect gate="P" pin="+VS" pad="13"/>
<connect gate="P" pin="-VS" pad="6"/>
<connect gate="P" pin="IN+" pad="5"/>
<connect gate="P" pin="IN-" pad="4"/>
<connect gate="P" pin="OUT" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD826" prefix="IC">
<description>&lt;b&gt;High-Speed, Low-Power Dual Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD826.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD826AR"/>
<attribute name="OC_FARNELL" value="1651291"/>
<attribute name="OC_NEWARK" value="05F7688"/>
</technology>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD826ANZ"/>
<attribute name="OC_FARNELL" value="1438583"/>
<attribute name="OC_NEWARK" value="59K6530"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD845" prefix="IC">
<description>&lt;b&gt;Precision, 16 MHz CBFET Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD845.pdf</description>
<gates>
<gate name="P" symbol="OP_OFFSET+-VS"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OFF@1" pad="1"/>
<connect gate="P" pin="OFF@2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD845KNZ"/>
<attribute name="OC_FARNELL" value="9605649"/>
<attribute name="OC_NEWARK" value="59K6757"/>
</technology>
</technologies>
</device>
<device name="R16" package="SOIC16R">
<connects>
<connect gate="P" pin="+VS" pad="13"/>
<connect gate="P" pin="-VS" pad="6"/>
<connect gate="P" pin="IN+" pad="5"/>
<connect gate="P" pin="IN-" pad="4"/>
<connect gate="P" pin="OFF@1" pad="3"/>
<connect gate="P" pin="OFF@2" pad="14"/>
<connect gate="P" pin="OUT" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD845JR-16"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="05F7719"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8529" prefix="IC">
<description>&lt;b&gt;8 MHz Rail-to-Rail Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8519_8529.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8529ARZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K6807"/>
</technology>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1424141"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8519" prefix="IC">
<description>&lt;b&gt;8 MHz Rail-to-Rail Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8519_8529.pdf</description>
<gates>
<gate name="P" symbol="OP+-VS"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="P" pin="+VS" pad="7"/>
<connect gate="P" pin="-VS" pad="4"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="2"/>
<connect gate="P" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8519ARZ"/>
<attribute name="OC_FARNELL" value="9603840"/>
<attribute name="OC_NEWARK" value="19M8912"/>
</technology>
</technologies>
</device>
<device name="RJ" package="SOT23-5">
<connects>
<connect gate="P" pin="+VS" pad="5"/>
<connect gate="P" pin="-VS" pad="2"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="4"/>
<connect gate="P" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8519ARTZ-REEL7"/>
<attribute name="OC_FARNELL" value="1464960"/>
<attribute name="OC_NEWARK" value="59K6794"/>
</technology>
</technologies>
</device>
<device name="KS" package="SC70-5">
<connects>
<connect gate="P" pin="+VS" pad="5"/>
<connect gate="P" pin="-VS" pad="2"/>
<connect gate="P" pin="IN+" pad="3"/>
<connect gate="P" pin="IN-" pad="4"/>
<connect gate="P" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8541" prefix="IC">
<description>&lt;b&gt;General-Purpose CMOS Rail-to-Rail Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8541_8542_8544.pdf</description>
<gates>
<gate name="G$1" symbol="OP+-VS"/>
</gates>
<devices>
<device name="KS" package="SC70-5">
<connects>
<connect gate="G$1" pin="+VS" pad="5"/>
<connect gate="G$1" pin="-VS" pad="2"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8541AKSZ-REEL7"/>
<attribute name="OC_FARNELL" value="1333253"/>
<attribute name="OC_NEWARK" value="59K6818"/>
</technology>
</technologies>
</device>
<device name="RJ" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+VS" pad="5"/>
<connect gate="G$1" pin="-VS" pad="2"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8541ARTZ-REEL7"/>
<attribute name="OC_FARNELL" value="1464963"/>
<attribute name="OC_NEWARK" value="88H0268"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8541ARZ"/>
<attribute name="OC_FARNELL" value="9603859"/>
<attribute name="OC_NEWARK" value="31M4547"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8542" prefix="IC">
<description>&lt;b&gt;General-Purpose CMOS Rail-to-Rail Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8541_8542_8544.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8542ARZ-REEL"/>
<attribute name="OC_FARNELL" value="1424150"/>
<attribute name="OC_NEWARK" value="59K6827"/>
</technology>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8542ARZ"/>
<attribute name="OC_FARNELL" value="1464965"/>
<attribute name="OC_NEWARK" value="19M0965"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8542ARUZ"/>
<attribute name="OC_FARNELL" value="1333256"/>
<attribute name="OC_NEWARK" value="88H0269"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8544" prefix="IC">
<description>&lt;b&gt;General-Purpose CMOS Rail-to-Rail Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8541_8542_8544.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="C" symbol="OP"/>
<gate name="D" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO14">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="IN+" pad="10"/>
<connect gate="C" pin="IN-" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="IN+" pad="12"/>
<connect gate="D" pin="IN-" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8544ARZ"/>
<attribute name="OC_FARNELL" value="9425748"/>
<attribute name="OC_NEWARK" value="19M0966"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP14">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="IN+" pad="10"/>
<connect gate="C" pin="IN-" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="IN+" pad="12"/>
<connect gate="D" pin="IN-" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8544ARUZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P1001"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8597" prefix="IC">
<description>&lt;b&gt;Single and Dual, Ultralow Distortion, Ultralow Noise Op Amps&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8597_8599.pdf</description>
<gates>
<gate name="G$1" symbol="OP+-VS"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8597ARZ"/>
<attribute name="OC_FARNELL" value="1701258"/>
<attribute name="OC_NEWARK" value="19P8303"/>
</technology>
</technologies>
</device>
<device name="CP" package="LFCSP8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8599" prefix="IC">
<description>&lt;b&gt;Single and Dual, Ultralow Distortion, Ultralow Noise Op Amps&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8597_8599.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8599ARZ"/>
<attribute name="OC_FARNELL" value="1438872"/>
<attribute name="OC_NEWARK" value="34M5072"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8610" prefix="IC">
<description>&lt;b&gt;Precision, Very Low Noise, Low Input Bias Current, Wide Bandwidth JFET Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8610_8620.pdf</description>
<gates>
<gate name="G$1" symbol="OP_OFFSET+-VS"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8610BRZ"/>
<attribute name="OC_FARNELL" value="8621578"/>
<attribute name="OC_NEWARK" value="59K6944"/>
</technology>
</technologies>
</device>
<device name="MR" package="MSOP08">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8610ARMZ-REEL"/>
<attribute name="OC_FARNELL" value="1424175"/>
<attribute name="OC_NEWARK" value="59K6939"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8620" prefix="IC">
<description>&lt;b&gt;Precision, Very Low Noise, Low Input Bias Current, Wide Bandwidth JFET Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8610_8620.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8620ARZ"/>
<attribute name="OC_FARNELL" value="9994386"/>
<attribute name="OC_NEWARK" value="59K6972"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8614" prefix="IC">
<description>&lt;b&gt;Single and Quad 18 V Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8614_8644.pdf</description>
<gates>
<gate name="G$1" symbol="OP+-VS"/>
</gates>
<devices>
<device name="RJ" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+VS" pad="5"/>
<connect gate="G$1" pin="-VS" pad="2"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8614ARTZ-REEL7"/>
<attribute name="OC_FARNELL" value="1464998"/>
<attribute name="OC_NEWARK" value="88H0303"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8644" prefix="IC">
<description>&lt;b&gt;Single and Quad 18 V Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8614_8644.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="C" symbol="OP"/>
<gate name="D" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO14">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="IN+" pad="10"/>
<connect gate="C" pin="IN-" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="IN+" pad="12"/>
<connect gate="D" pin="IN-" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8644ARZ"/>
<attribute name="OC_FARNELL" value="1438873"/>
<attribute name="OC_NEWARK" value="59K7037"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP14">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="IN+" pad="10"/>
<connect gate="C" pin="IN-" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="IN+" pad="12"/>
<connect gate="D" pin="IN-" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8644ARUZ"/>
<attribute name="OC_FARNELL" value="1438873"/>
<attribute name="OC_NEWARK" value="59K7036"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8656" prefix="IC">
<description>&lt;b&gt;Low Noise, Precision CMOS Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8655_8656.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="RM" package="MSOP08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8656ARMZ"/>
<attribute name="OC_FARNELL" value="1117887"/>
<attribute name="OC_NEWARK" value="34P3252"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8656ARZ"/>
<attribute name="OC_FARNELL" value="1117887"/>
<attribute name="OC_NEWARK" value="19M0993"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8655" prefix="IC">
<description>&lt;b&gt;Low Noise, Precision CMOS Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8655_8656.pdf</description>
<gates>
<gate name="G$1" symbol="OP+-VS"/>
</gates>
<devices>
<device name="RM" package="MSOP08">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8655ARZ"/>
<attribute name="OC_FARNELL" value="1078267"/>
<attribute name="OC_NEWARK" value="59K7052"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8655ARMZ-REEL"/>
<attribute name="OC_FARNELL" value="1078267"/>
<attribute name="OC_NEWARK" value="59K7050"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4075-2" prefix="IC">
<description>&lt;b&gt;Ultralow Noise Amplifier at Lower Power&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4075-2.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADA4075-2ARZ"/>
<attribute name="OC_FARNELL" value="1701254"/>
<attribute name="OC_NEWARK" value="19P8164"/>
</technology>
</technologies>
</device>
<device name="CP" package="LFCSP8_CP">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADA4075-2ACPZ-R7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="26R2389"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4627-1R" prefix="IC">
<description>&lt;b&gt;36 V, 19 MHz, Low Noise, Low Bias Current, JFET Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4627-1.pdf</description>
<gates>
<gate name="G$1" symbol="OP_OFFSET+-VS"/>
</gates>
<devices>
<device name="" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADA4627-1ARZ"/>
<attribute name="OC_FARNELL" value="1827378"/>
<attribute name="OC_NEWARK" value="26R2398"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4627-1CP" prefix="IC">
<description>&lt;b&gt;36 V, 19 MHz, Low Noise, Low Bias Current, JFET Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4627-1.pdf</description>
<gates>
<gate name="G$1" symbol="OP+-VS"/>
</gates>
<devices>
<device name="" package="LFCSP8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADA4627-1ACPZ-R2"/>
<attribute name="OC_FARNELL" value="1827379"/>
<attribute name="OC_NEWARK" value="80R8148"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4692-4" prefix="IC">
<description>&lt;b&gt;Low Power, 3.6 MHz, Low Noise, Rail-to-Rail Output, Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4691-2_4692-2_4692-4.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="C" symbol="OP"/>
<gate name="D" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="RU" package="TSSOP14">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="IN+" pad="10"/>
<connect gate="C" pin="IN-" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="IN+" pad="12"/>
<connect gate="D" pin="IN-" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADA4692-4ARUZ"/>
<attribute name="OC_FARNELL" value="1827393"/>
<attribute name="OC_NEWARK" value="80R8154"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4692-2" prefix="IC">
<description>&lt;b&gt;Low Power, 3.6 MHz, Low Noise, Rail-to-Rail Output, Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4691-2_4692-2_4692-4.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADA4692-2ARZ"/>
<attribute name="OC_FARNELL" value="1760810"/>
<attribute name="OC_NEWARK" value="05R6523"/>
</technology>
</technologies>
</device>
<device name="CP" package="LFCSP8_CP">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1827383"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4853-2" prefix="IC">
<description>&lt;b&gt;Low Power, Rail-to-Rail Output, Video Op Amps with Ultralow Power&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4853-1_4853-2_4853-3.pdf</description>
<gates>
<gate name="A" symbol="OP_PD"/>
<gate name="B" symbol="OP_PD"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="VQ" package="LFCSP16">
<connects>
<connect gate="A" pin="!POWERDOWN" pad="14"/>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="!POWERDOWN" pad="13"/>
<connect gate="B" pin="IN+" pad="9"/>
<connect gate="B" pin="IN-" pad="10"/>
<connect gate="B" pin="OUT" pad="11"/>
<connect gate="P" pin="V+" pad="12"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4853-1" prefix="IC">
<description>&lt;b&gt;Low Power, Rail-to-Rail Output, Video Op Amps with Ultralow Power&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4853-1_4853-2_4853-3.pdf</description>
<gates>
<gate name="G$1" symbol="OP_PD"/>
<gate name="G$2" symbol="PWR+-"/>
</gates>
<devices>
<device name="" package="SC70-6">
<connects>
<connect gate="G$1" pin="!POWERDOWN" pad="5"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$2" pin="V+" pad="6"/>
<connect gate="G$2" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4853-3VQ" prefix="IC">
<description>&lt;b&gt;Low Power, Rail-to-Rail Output, Video Op Amps with Ultralow Power&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4853-1_4853-2_4853-3.pdf</description>
<gates>
<gate name="A" symbol="OP_PD"/>
<gate name="B" symbol="OP_PD"/>
<gate name="C" symbol="OP_PD"/>
<gate name="P" symbol="PWR+-2"/>
</gates>
<devices>
<device name="" package="LFCSP16">
<connects>
<connect gate="A" pin="!POWERDOWN" pad="1"/>
<connect gate="A" pin="IN+" pad="5"/>
<connect gate="A" pin="IN-" pad="6"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="B" pin="!POWERDOWN" pad="2"/>
<connect gate="B" pin="IN+" pad="11"/>
<connect gate="B" pin="IN-" pad="10"/>
<connect gate="B" pin="OUT" pad="9"/>
<connect gate="C" pin="!POWERDOWN" pad="3"/>
<connect gate="C" pin="IN+" pad="13"/>
<connect gate="C" pin="IN-" pad="14"/>
<connect gate="C" pin="OUT" pad="15"/>
<connect gate="P" pin="V+@1" pad="4"/>
<connect gate="P" pin="V+@2" pad="16"/>
<connect gate="P" pin="V-@1" pad="8"/>
<connect gate="P" pin="V-@2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADA4853-3RU" prefix="IC">
<description>&lt;b&gt;Low Power, Rail-to-Rail Output, Video Op Amps with Ultralow Power&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADA4853-1_4853-2_4853-3.pdf</description>
<gates>
<gate name="A" symbol="OP_PD"/>
<gate name="B" symbol="OP_PD"/>
<gate name="C" symbol="OP_PD"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="A" pin="!POWERDOWN" pad="1"/>
<connect gate="A" pin="IN+" pad="5"/>
<connect gate="A" pin="IN-" pad="6"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="B" pin="!POWERDOWN" pad="2"/>
<connect gate="B" pin="IN+" pad="10"/>
<connect gate="B" pin="IN-" pad="9"/>
<connect gate="B" pin="OUT" pad="8"/>
<connect gate="C" pin="!POWERDOWN" pad="3"/>
<connect gate="C" pin="IN+" pad="12"/>
<connect gate="C" pin="IN-" pad="13"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADA4853-3YRUZ"/>
<attribute name="OC_FARNELL" value="1498692"/>
<attribute name="OC_NEWARK" value="15P0326"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADAU1592" prefix="IC">
<description>&lt;b&gt;Class-D Audio Power Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADAU1592.pdf</description>
<gates>
<gate name="G$1" symbol="ADAU1592"/>
</gates>
<devices>
<device name="SV" package="QFP-7X7-48">
<connects>
<connect gate="G$1" pin="!ERR" pad="9"/>
<connect gate="G$1" pin="!MUTE" pad="15"/>
<connect gate="G$1" pin="!OTW" pad="10"/>
<connect gate="G$1" pin="!STDN" pad="16"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AINL" pad="27"/>
<connect gate="G$1" pin="AINR" pad="28"/>
<connect gate="G$1" pin="AVDD" pad="21"/>
<connect gate="G$1" pin="DGND" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="MO/!ST" pad="11"/>
<connect gate="G$1" pin="OUTL+@1" pad="4"/>
<connect gate="G$1" pin="OUTL+@2" pad="5"/>
<connect gate="G$1" pin="OUTL+@3" pad="6"/>
<connect gate="G$1" pin="OUTL-@1" pad="1"/>
<connect gate="G$1" pin="OUTL-@2" pad="2"/>
<connect gate="G$1" pin="OUTL-@3" pad="3"/>
<connect gate="G$1" pin="OUTR+@1" pad="31"/>
<connect gate="G$1" pin="OUTR+@2" pad="32"/>
<connect gate="G$1" pin="OUTR+@3" pad="33"/>
<connect gate="G$1" pin="OUTR-@1" pad="35"/>
<connect gate="G$1" pin="OUTR-@2" pad="36"/>
<connect gate="G$1" pin="OUTR-@3" pad="37"/>
<connect gate="G$1" pin="PGA0" pad="14"/>
<connect gate="G$1" pin="PGA1" pad="13"/>
<connect gate="G$1" pin="PGND@1" pad="34"/>
<connect gate="G$1" pin="PGND@2" pad="38"/>
<connect gate="G$1" pin="PGND@3" pad="47"/>
<connect gate="G$1" pin="PGND@4" pad="48"/>
<connect gate="G$1" pin="PVDD@1" pad="39"/>
<connect gate="G$1" pin="PVDD@2" pad="40"/>
<connect gate="G$1" pin="PVDD@3" pad="41"/>
<connect gate="G$1" pin="PVDD@4" pad="42"/>
<connect gate="G$1" pin="PVDD@5" pad="43"/>
<connect gate="G$1" pin="PVDD@6" pad="44"/>
<connect gate="G$1" pin="PVDD@7" pad="45"/>
<connect gate="G$1" pin="PVDD@8" pad="46"/>
<connect gate="G$1" pin="SLC_TH" pad="24"/>
<connect gate="G$1" pin="TEST0" pad="8"/>
<connect gate="G$1" pin="TEST1" pad="7"/>
<connect gate="G$1" pin="TEST12" pad="29"/>
<connect gate="G$1" pin="TEST13" pad="30"/>
<connect gate="G$1" pin="TEST3" pad="12"/>
<connect gate="G$1" pin="TEST8" pad="25"/>
<connect gate="G$1" pin="TEST9" pad="26"/>
<connect gate="G$1" pin="VREF" pad="23"/>
<connect gate="G$1" pin="XTI" pad="17"/>
<connect gate="G$1" pin="XTO" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1498683"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="CP" package="LFCSP48">
<connects>
<connect gate="G$1" pin="!ERR" pad="9"/>
<connect gate="G$1" pin="!MUTE" pad="15"/>
<connect gate="G$1" pin="!OTW" pad="10"/>
<connect gate="G$1" pin="!STDN" pad="16"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AINL" pad="27"/>
<connect gate="G$1" pin="AINR" pad="28"/>
<connect gate="G$1" pin="AVDD" pad="21"/>
<connect gate="G$1" pin="DGND" pad="19"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="MO/!ST" pad="11"/>
<connect gate="G$1" pin="OUTL+@1" pad="4"/>
<connect gate="G$1" pin="OUTL+@2" pad="5"/>
<connect gate="G$1" pin="OUTL+@3" pad="6"/>
<connect gate="G$1" pin="OUTL-@1" pad="1"/>
<connect gate="G$1" pin="OUTL-@2" pad="2"/>
<connect gate="G$1" pin="OUTL-@3" pad="3"/>
<connect gate="G$1" pin="OUTR+@1" pad="31"/>
<connect gate="G$1" pin="OUTR+@2" pad="32"/>
<connect gate="G$1" pin="OUTR+@3" pad="33"/>
<connect gate="G$1" pin="OUTR-@1" pad="35"/>
<connect gate="G$1" pin="OUTR-@2" pad="36"/>
<connect gate="G$1" pin="OUTR-@3" pad="37"/>
<connect gate="G$1" pin="PGA0" pad="14"/>
<connect gate="G$1" pin="PGA1" pad="13"/>
<connect gate="G$1" pin="PGND@1" pad="34"/>
<connect gate="G$1" pin="PGND@2" pad="38"/>
<connect gate="G$1" pin="PGND@3" pad="47"/>
<connect gate="G$1" pin="PGND@4" pad="48"/>
<connect gate="G$1" pin="PVDD@1" pad="39"/>
<connect gate="G$1" pin="PVDD@2" pad="40"/>
<connect gate="G$1" pin="PVDD@3" pad="41"/>
<connect gate="G$1" pin="PVDD@4" pad="42"/>
<connect gate="G$1" pin="PVDD@5" pad="43"/>
<connect gate="G$1" pin="PVDD@6" pad="44"/>
<connect gate="G$1" pin="PVDD@7" pad="45"/>
<connect gate="G$1" pin="PVDD@8" pad="46"/>
<connect gate="G$1" pin="SLC_TH" pad="24"/>
<connect gate="G$1" pin="TEST0" pad="8"/>
<connect gate="G$1" pin="TEST1" pad="7"/>
<connect gate="G$1" pin="TEST12" pad="29"/>
<connect gate="G$1" pin="TEST13" pad="30"/>
<connect gate="G$1" pin="TEST3" pad="12"/>
<connect gate="G$1" pin="TEST8" pad="25"/>
<connect gate="G$1" pin="TEST9" pad="26"/>
<connect gate="G$1" pin="VREF" pad="23"/>
<connect gate="G$1" pin="XTI" pad="17"/>
<connect gate="G$1" pin="XTO" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADAU1592ACPZ"/>
<attribute name="OC_FARNELL" value="1498683"/>
<attribute name="OC_NEWARK" value="50M0756"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADAV801" prefix="IC">
<description>&lt;b&gt;Audio Codec for Recordable DVD&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADAV801.pdf</description>
<gates>
<gate name="G$1" symbol="ADAV801"/>
</gates>
<devices>
<device name="ST" package="LQFP-ST-64-2">
<connects>
<connect gate="G$1" pin="ADGND" pad="47"/>
<connect gate="G$1" pin="ADVDD" pad="48"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AGND@1" pad="54"/>
<connect gate="G$1" pin="AGND@2" pad="56"/>
<connect gate="G$1" pin="AGND@3" pad="58"/>
<connect gate="G$1" pin="AGND@4" pad="62"/>
<connect gate="G$1" pin="AVDD" pad="4"/>
<connect gate="G$1" pin="AVDD@1" pad="53"/>
<connect gate="G$1" pin="AVDD@2" pad="59"/>
<connect gate="G$1" pin="CAPLN" pad="64"/>
<connect gate="G$1" pin="CAPLP" pad="63"/>
<connect gate="G$1" pin="CAPRN" pad="60"/>
<connect gate="G$1" pin="CAPRP" pad="61"/>
<connect gate="G$1" pin="CCLK" pad="11"/>
<connect gate="G$1" pin="CIN" pad="10"/>
<connect gate="G$1" pin="CLATCH" pad="9"/>
<connect gate="G$1" pin="COUT" pad="12"/>
<connect gate="G$1" pin="DGND" pad="16"/>
<connect gate="G$1" pin="DGND@1" pad="33"/>
<connect gate="G$1" pin="DGND@2" pad="42"/>
<connect gate="G$1" pin="DIRIN" pad="23"/>
<connect gate="G$1" pin="DIR_GND" pad="6"/>
<connect gate="G$1" pin="DIR_LF" pad="5"/>
<connect gate="G$1" pin="DIR_VDD" pad="7"/>
<connect gate="G$1" pin="DITOUT" pad="26"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="DVDD@1" pad="34"/>
<connect gate="G$1" pin="FILTD" pad="55"/>
<connect gate="G$1" pin="IAUXBCLK" pad="31"/>
<connect gate="G$1" pin="IAUXLRCLK" pad="30"/>
<connect gate="G$1" pin="IAUXSDATA" pad="32"/>
<connect gate="G$1" pin="IBCLK" pad="18"/>
<connect gate="G$1" pin="ILRCLK" pad="17"/>
<connect gate="G$1" pin="ISDATA" pad="19"/>
<connect gate="G$1" pin="MCLKI" pad="35"/>
<connect gate="G$1" pin="MCLKO" pad="36"/>
<connect gate="G$1" pin="NC" pad="50"/>
<connect gate="G$1" pin="NC@1" pad="52"/>
<connect gate="G$1" pin="OAUXBCLK" pad="28"/>
<connect gate="G$1" pin="OAUXLRCLK" pad="27"/>
<connect gate="G$1" pin="OAUXSDATA" pad="29"/>
<connect gate="G$1" pin="OBCLK" pad="21"/>
<connect gate="G$1" pin="ODGND" pad="25"/>
<connect gate="G$1" pin="ODVDD" pad="24"/>
<connect gate="G$1" pin="OLRCLK" pad="20"/>
<connect gate="G$1" pin="OSDATA" pad="22"/>
<connect gate="G$1" pin="PLL_GND" pad="44"/>
<connect gate="G$1" pin="PLL_LF1" pad="45"/>
<connect gate="G$1" pin="PLL_LF2" pad="46"/>
<connect gate="G$1" pin="PLL_VDD" pad="43"/>
<connect gate="G$1" pin="RESET" pad="8"/>
<connect gate="G$1" pin="SYSCLK1" pad="41"/>
<connect gate="G$1" pin="SYSCLK2" pad="40"/>
<connect gate="G$1" pin="SYSCLK3" pad="39"/>
<connect gate="G$1" pin="VINL" pad="2"/>
<connect gate="G$1" pin="VINR" pad="1"/>
<connect gate="G$1" pin="VOUTL" pad="51"/>
<connect gate="G$1" pin="VOUTR" pad="49"/>
<connect gate="G$1" pin="VREF" pad="57"/>
<connect gate="G$1" pin="XIN" pad="38"/>
<connect gate="G$1" pin="XOUT" pad="37"/>
<connect gate="G$1" pin="ZEROL/INT" pad="13"/>
<connect gate="G$1" pin="ZEROR" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADAV801ASTZ"/>
<attribute name="OC_FARNELL" value="1438741"/>
<attribute name="OC_NEWARK" value="26R5500"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADAV803" prefix="IC">
<description>&lt;b&gt;Audio Codec for Recordable DVD&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADAV803.pdf</description>
<gates>
<gate name="G$1" symbol="ADAV803"/>
</gates>
<devices>
<device name="" package="LQFP-ST-64-2">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="AD1" pad="12"/>
<connect gate="G$1" pin="ADGND" pad="47"/>
<connect gate="G$1" pin="ADVDD" pad="48"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AGND@1" pad="54"/>
<connect gate="G$1" pin="AGND@2" pad="56"/>
<connect gate="G$1" pin="AGND@3" pad="58"/>
<connect gate="G$1" pin="AGND@4" pad="62"/>
<connect gate="G$1" pin="AVDD" pad="4"/>
<connect gate="G$1" pin="AVDD@1" pad="53"/>
<connect gate="G$1" pin="AVDD@2" pad="59"/>
<connect gate="G$1" pin="CAPLN" pad="64"/>
<connect gate="G$1" pin="CAPLP" pad="63"/>
<connect gate="G$1" pin="CAPRN" pad="60"/>
<connect gate="G$1" pin="CAPRP" pad="61"/>
<connect gate="G$1" pin="DGND" pad="16"/>
<connect gate="G$1" pin="DGND@1" pad="33"/>
<connect gate="G$1" pin="DGND@2" pad="42"/>
<connect gate="G$1" pin="DIRIN" pad="23"/>
<connect gate="G$1" pin="DIR_GND" pad="6"/>
<connect gate="G$1" pin="DIR_LF" pad="5"/>
<connect gate="G$1" pin="DIR_VDD" pad="7"/>
<connect gate="G$1" pin="DITOUT" pad="26"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="DVDD@1" pad="34"/>
<connect gate="G$1" pin="FILTD" pad="55"/>
<connect gate="G$1" pin="IAUXBCLK" pad="31"/>
<connect gate="G$1" pin="IAUXLRCLK" pad="30"/>
<connect gate="G$1" pin="IAUXSDATA" pad="32"/>
<connect gate="G$1" pin="IBCLK" pad="18"/>
<connect gate="G$1" pin="ILRCLK" pad="17"/>
<connect gate="G$1" pin="ISDATA" pad="19"/>
<connect gate="G$1" pin="MCLKI" pad="35"/>
<connect gate="G$1" pin="MCLKO" pad="36"/>
<connect gate="G$1" pin="NC" pad="50"/>
<connect gate="G$1" pin="NC@1" pad="52"/>
<connect gate="G$1" pin="OAUXBCLK" pad="28"/>
<connect gate="G$1" pin="OAUXLRCLK" pad="27"/>
<connect gate="G$1" pin="OAUXSDATA" pad="29"/>
<connect gate="G$1" pin="OBCLK" pad="21"/>
<connect gate="G$1" pin="ODGND" pad="25"/>
<connect gate="G$1" pin="ODVDD" pad="24"/>
<connect gate="G$1" pin="OLRCLK" pad="20"/>
<connect gate="G$1" pin="OSDATA" pad="22"/>
<connect gate="G$1" pin="PLL_GND" pad="44"/>
<connect gate="G$1" pin="PLL_LF1" pad="45"/>
<connect gate="G$1" pin="PLL_LF2" pad="46"/>
<connect gate="G$1" pin="PLL_VDD" pad="43"/>
<connect gate="G$1" pin="RESET" pad="8"/>
<connect gate="G$1" pin="SCL" pad="11"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="SYSCLK1" pad="41"/>
<connect gate="G$1" pin="SYSCLK2" pad="40"/>
<connect gate="G$1" pin="SYSCLK3" pad="39"/>
<connect gate="G$1" pin="VINL" pad="2"/>
<connect gate="G$1" pin="VINR" pad="1"/>
<connect gate="G$1" pin="VOUTL" pad="51"/>
<connect gate="G$1" pin="VOUTR" pad="49"/>
<connect gate="G$1" pin="VREF" pad="57"/>
<connect gate="G$1" pin="XIN" pad="38"/>
<connect gate="G$1" pin="XOUT" pad="37"/>
<connect gate="G$1" pin="ZEROL/INT" pad="13"/>
<connect gate="G$1" pin="ZEROR" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADAV803ASTZ-REEL"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K0877"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADAV804" prefix="IC">
<description>&lt;b&gt;Audio Codec For Recordable DVD&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADAV804.pdf</description>
<gates>
<gate name="G$1" symbol="ADAV804"/>
</gates>
<devices>
<device name="" package="LQFP-ST-64-2">
<connects>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="AD1" pad="12"/>
<connect gate="G$1" pin="ADGND" pad="47"/>
<connect gate="G$1" pin="ADVDD" pad="48"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AGND@1" pad="54"/>
<connect gate="G$1" pin="AGND@2" pad="56"/>
<connect gate="G$1" pin="AGND@3" pad="58"/>
<connect gate="G$1" pin="AGND@4" pad="62"/>
<connect gate="G$1" pin="AVDD" pad="4"/>
<connect gate="G$1" pin="AVDD@1" pad="53"/>
<connect gate="G$1" pin="AVDD@2" pad="59"/>
<connect gate="G$1" pin="CAPLN" pad="64"/>
<connect gate="G$1" pin="CAPLP" pad="63"/>
<connect gate="G$1" pin="CAPRN" pad="60"/>
<connect gate="G$1" pin="CAPRP" pad="61"/>
<connect gate="G$1" pin="DGND" pad="16"/>
<connect gate="G$1" pin="DGND@1" pad="33"/>
<connect gate="G$1" pin="DGND@2" pad="42"/>
<connect gate="G$1" pin="DIRIN" pad="23"/>
<connect gate="G$1" pin="DIR_GND" pad="6"/>
<connect gate="G$1" pin="DIR_LF" pad="5"/>
<connect gate="G$1" pin="DIR_VDD" pad="7"/>
<connect gate="G$1" pin="DITOUT" pad="26"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="DVDD@1" pad="34"/>
<connect gate="G$1" pin="FILTD" pad="55"/>
<connect gate="G$1" pin="IAUXBCLK" pad="31"/>
<connect gate="G$1" pin="IAUXLRCLK" pad="30"/>
<connect gate="G$1" pin="IAUXSDATA" pad="32"/>
<connect gate="G$1" pin="IBCLK" pad="18"/>
<connect gate="G$1" pin="ILRCLK" pad="17"/>
<connect gate="G$1" pin="ISDATA" pad="19"/>
<connect gate="G$1" pin="MCLKI" pad="35"/>
<connect gate="G$1" pin="MCLKO" pad="36"/>
<connect gate="G$1" pin="NC" pad="50"/>
<connect gate="G$1" pin="NC@1" pad="52"/>
<connect gate="G$1" pin="OAUXBCLK" pad="28"/>
<connect gate="G$1" pin="OAUXLRCLK" pad="27"/>
<connect gate="G$1" pin="OAUXSDATA" pad="29"/>
<connect gate="G$1" pin="OBCLK" pad="21"/>
<connect gate="G$1" pin="ODGND" pad="25"/>
<connect gate="G$1" pin="ODVDD" pad="24"/>
<connect gate="G$1" pin="OLRCLK" pad="20"/>
<connect gate="G$1" pin="OSDATA" pad="22"/>
<connect gate="G$1" pin="OUTPUT" pad="51"/>
<connect gate="G$1" pin="PLL_GND" pad="44"/>
<connect gate="G$1" pin="PLL_LF1" pad="45"/>
<connect gate="G$1" pin="PLL_LF2" pad="46"/>
<connect gate="G$1" pin="PLL_VDD" pad="43"/>
<connect gate="G$1" pin="RESET" pad="8"/>
<connect gate="G$1" pin="SCL" pad="11"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="SYSCLK1" pad="41"/>
<connect gate="G$1" pin="SYSCLK2" pad="40"/>
<connect gate="G$1" pin="SYSCLK3" pad="39"/>
<connect gate="G$1" pin="VINL" pad="2"/>
<connect gate="G$1" pin="VINR" pad="1"/>
<connect gate="G$1" pin="VOUTR" pad="49"/>
<connect gate="G$1" pin="VREF" pad="57"/>
<connect gate="G$1" pin="XIN" pad="38"/>
<connect gate="G$1" pin="XOUT" pad="37"/>
<connect gate="G$1" pin="ZEROL/INT" pad="13"/>
<connect gate="G$1" pin="ZEROR" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG412" prefix="IC">
<description>&lt;b&gt;LC2MOS Precision Quad SPST Switches&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADG411_412_413.pdf</description>
<gates>
<gate name="A" symbol="ADG-SWITCH-OPEN"/>
<gate name="B" symbol="ADG-SWITCH-OPEN"/>
<gate name="C" symbol="ADG-SWITCH-OPEN"/>
<gate name="D" symbol="ADG-SWITCH-OPEN"/>
<gate name="P" symbol="PWR-VSS-VDD-GND-VL"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG412TQ"/>
<attribute name="OC_FARNELL" value="1438704"/>
<attribute name="OC_NEWARK" value="09B7025"/>
</technology>
</technologies>
</device>
<device name="R" package="SOIC16N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG412BRZ"/>
<attribute name="OC_FARNELL" value="1661021"/>
<attribute name="OC_NEWARK" value="59K1252"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG412BRU-REEL7"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59K1251"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG411" prefix="IC">
<description>&lt;b&gt;LC2MOS Precision Quad SPST Switches&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADG411_412_413.pdf</description>
<gates>
<gate name="A" symbol="ADG-SWITCH-CLOSE-INV"/>
<gate name="B" symbol="ADG-SWITCH-CLOSE-INV"/>
<gate name="C" symbol="ADG-SWITCH-CLOSE-INV"/>
<gate name="D" symbol="ADG-SWITCH-CLOSE-INV"/>
<gate name="P" symbol="PWR-VSS-VDD-GND-VL"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG411BN"/>
<attribute name="OC_FARNELL" value="1424317"/>
<attribute name="OC_NEWARK" value="05F6198"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="ADG411BRUZ"/>
<attribute name="OC_FARNELL" value="1424318"/>
<attribute name="OC_NEWARK" value="59K1243"/>
</technology>
</technologies>
</device>
<device name="R" package="SOIC16N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG411BRZ"/>
<attribute name="OC_FARNELL" value="1424319"/>
<attribute name="OC_NEWARK" value="19M8649"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG413" prefix="IC">
<description>&lt;b&gt;LC2MOS Precision Quad SPST Switches&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADG411_412_413.pdf</description>
<gates>
<gate name="A" symbol="ADG-SWITCH-OPEN"/>
<gate name="B" symbol="ADG-SWITCH-CLOSE-INV"/>
<gate name="C" symbol="ADG-SWITCH-CLOSE-INV"/>
<gate name="D" symbol="ADG-SWITCH-OPEN"/>
<gate name="P" symbol="PWR-VSS-VDD-GND-VL"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG413BNZ"/>
<attribute name="OC_FARNELL" value="1079411"/>
<attribute name="OC_NEWARK" value="31M3784"/>
</technology>
</technologies>
</device>
<device name="R" package="SOIC16N">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADG413BRZ"/>
<attribute name="OC_FARNELL" value="1465179"/>
<attribute name="OC_NEWARK" value="19M8650"/>
</technology>
</technologies>
</device>
<device name="RU" package="TSSOP16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VDD" pad="13"/>
<connect gate="P" pin="VL" pad="12"/>
<connect gate="P" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1319241"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_21368" prefix="IC">
<description>&lt;b&gt;SHARC Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: 78445023821368_256ballSBGA_bsdl_PrA_0206.txt&lt;br&gt;
http://www.analog.com/static/imported-files/data_sheets/ADSP-21367_21368_21369.pdf</description>
<gates>
<gate name="G$1" symbol="ADSP_21368"/>
</gates>
<devices>
<device name="" package="BGA_256">
<connects>
<connect gate="G$1" pin="ACK" pad="M1"/>
<connect gate="G$1" pin="ADDR0" pad="W19"/>
<connect gate="G$1" pin="ADDR1" pad="W17"/>
<connect gate="G$1" pin="ADDR10" pad="W13"/>
<connect gate="G$1" pin="ADDR11" pad="Y13"/>
<connect gate="G$1" pin="ADDR12" pad="W12"/>
<connect gate="G$1" pin="ADDR13" pad="W11"/>
<connect gate="G$1" pin="ADDR14" pad="W8"/>
<connect gate="G$1" pin="ADDR15" pad="W7"/>
<connect gate="G$1" pin="ADDR16" pad="W6"/>
<connect gate="G$1" pin="ADDR17" pad="W5"/>
<connect gate="G$1" pin="ADDR18" pad="Y4"/>
<connect gate="G$1" pin="ADDR19" pad="W3"/>
<connect gate="G$1" pin="ADDR2" pad="W18"/>
<connect gate="G$1" pin="ADDR20" pad="W4"/>
<connect gate="G$1" pin="ADDR21" pad="W2"/>
<connect gate="G$1" pin="ADDR22" pad="V1"/>
<connect gate="G$1" pin="ADDR23" pad="V2"/>
<connect gate="G$1" pin="ADDR3" pad="Y17"/>
<connect gate="G$1" pin="ADDR4" pad="W16"/>
<connect gate="G$1" pin="ADDR5" pad="W15"/>
<connect gate="G$1" pin="ADDR6" pad="Y16"/>
<connect gate="G$1" pin="ADDR7" pad="Y15"/>
<connect gate="G$1" pin="ADDR8" pad="W14"/>
<connect gate="G$1" pin="ADDR9" pad="Y14"/>
<connect gate="G$1" pin="AVDD" pad="W9"/>
<connect gate="G$1" pin="AVSS" pad="W10"/>
<connect gate="G$1" pin="BOOTCFG0" pad="B5"/>
<connect gate="G$1" pin="BOOTCFG1" pad="B6"/>
<connect gate="G$1" pin="BR1_B" pad="Y5"/>
<connect gate="G$1" pin="BR2_B" pad="Y6"/>
<connect gate="G$1" pin="BR3_B" pad="Y11"/>
<connect gate="G$1" pin="BR4_B" pad="Y12"/>
<connect gate="G$1" pin="CLKIN" pad="Y8"/>
<connect gate="G$1" pin="CLKOUT" pad="A17"/>
<connect gate="G$1" pin="CLK_CFG0" pad="A4"/>
<connect gate="G$1" pin="CLK_CFG1" pad="A5"/>
<connect gate="G$1" pin="DAI1" pad="A8"/>
<connect gate="G$1" pin="DAI10" pad="D1"/>
<connect gate="G$1" pin="DAI11" pad="E1"/>
<connect gate="G$1" pin="DAI12" pad="F2"/>
<connect gate="G$1" pin="DAI13" pad="G2"/>
<connect gate="G$1" pin="DAI14" pad="F1"/>
<connect gate="G$1" pin="DAI15" pad="G1"/>
<connect gate="G$1" pin="DAI16" pad="H2"/>
<connect gate="G$1" pin="DAI17" pad="H1"/>
<connect gate="G$1" pin="DAI18" pad="J2"/>
<connect gate="G$1" pin="DAI19" pad="J1"/>
<connect gate="G$1" pin="DAI2" pad="B9"/>
<connect gate="G$1" pin="DAI20" pad="K2"/>
<connect gate="G$1" pin="DAI3" pad="B8"/>
<connect gate="G$1" pin="DAI4" pad="A7"/>
<connect gate="G$1" pin="DAI5" pad="B1"/>
<connect gate="G$1" pin="DAI6" pad="D2"/>
<connect gate="G$1" pin="DAI7" pad="C2"/>
<connect gate="G$1" pin="DAI8" pad="E2"/>
<connect gate="G$1" pin="DAI9" pad="C1"/>
<connect gate="G$1" pin="DATA0" pad="U19"/>
<connect gate="G$1" pin="DATA1" pad="V19"/>
<connect gate="G$1" pin="DATA10" pad="N20"/>
<connect gate="G$1" pin="DATA11" pad="N19"/>
<connect gate="G$1" pin="DATA12" pad="M19"/>
<connect gate="G$1" pin="DATA13" pad="M20"/>
<connect gate="G$1" pin="DATA14" pad="L20"/>
<connect gate="G$1" pin="DATA15" pad="L19"/>
<connect gate="G$1" pin="DATA16" pad="K20"/>
<connect gate="G$1" pin="DATA17" pad="J20"/>
<connect gate="G$1" pin="DATA18" pad="H20"/>
<connect gate="G$1" pin="DATA19" pad="H19"/>
<connect gate="G$1" pin="DATA2" pad="U20"/>
<connect gate="G$1" pin="DATA20" pad="G20"/>
<connect gate="G$1" pin="DATA21" pad="F20"/>
<connect gate="G$1" pin="DATA22" pad="G19"/>
<connect gate="G$1" pin="DATA23" pad="E20"/>
<connect gate="G$1" pin="DATA24" pad="D20"/>
<connect gate="G$1" pin="DATA25" pad="E19"/>
<connect gate="G$1" pin="DATA26" pad="D19"/>
<connect gate="G$1" pin="DATA27" pad="C19"/>
<connect gate="G$1" pin="DATA28" pad="B19"/>
<connect gate="G$1" pin="DATA29" pad="B18"/>
<connect gate="G$1" pin="DATA3" pad="V20"/>
<connect gate="G$1" pin="DATA30" pad="B17"/>
<connect gate="G$1" pin="DATA31" pad="A18"/>
<connect gate="G$1" pin="DATA4" pad="T20"/>
<connect gate="G$1" pin="DATA5" pad="T19"/>
<connect gate="G$1" pin="DATA6" pad="R19"/>
<connect gate="G$1" pin="DATA7" pad="R20"/>
<connect gate="G$1" pin="DATA8" pad="P19"/>
<connect gate="G$1" pin="DATA9" pad="P20"/>
<connect gate="G$1" pin="DPI1" pad="B15"/>
<connect gate="G$1" pin="DPI10" pad="A11"/>
<connect gate="G$1" pin="DPI11" pad="B11"/>
<connect gate="G$1" pin="DPI12" pad="A10"/>
<connect gate="G$1" pin="DPI13" pad="B10"/>
<connect gate="G$1" pin="DPI14" pad="A9"/>
<connect gate="G$1" pin="DPI2" pad="A16"/>
<connect gate="G$1" pin="DPI3" pad="A15"/>
<connect gate="G$1" pin="DPI4" pad="B14"/>
<connect gate="G$1" pin="DPI5" pad="B13"/>
<connect gate="G$1" pin="DPI6" pad="A14"/>
<connect gate="G$1" pin="DPI7" pad="A13"/>
<connect gate="G$1" pin="DPI8" pad="B12"/>
<connect gate="G$1" pin="DPI9" pad="A12"/>
<connect gate="G$1" pin="EMU_B" pad="A6"/>
<connect gate="G$1" pin="FLAG0" pad="K1"/>
<connect gate="G$1" pin="FLAG1" pad="L2"/>
<connect gate="G$1" pin="FLAG2" pad="L1"/>
<connect gate="G$1" pin="FLAG3" pad="M2"/>
<connect gate="G$1" pin="GND@0" pad="C3"/>
<connect gate="G$1" pin="GND@1" pad="C5"/>
<connect gate="G$1" pin="GND@10" pad="D5"/>
<connect gate="G$1" pin="GND@11" pad="D8"/>
<connect gate="G$1" pin="GND@12" pad="D11"/>
<connect gate="G$1" pin="GND@13" pad="D14"/>
<connect gate="G$1" pin="GND@14" pad="D16"/>
<connect gate="G$1" pin="GND@15" pad="D18"/>
<connect gate="G$1" pin="GND@16" pad="E17"/>
<connect gate="G$1" pin="GND@17" pad="E18"/>
<connect gate="G$1" pin="GND@18" pad="F3"/>
<connect gate="G$1" pin="GND@19" pad="F4"/>
<connect gate="G$1" pin="GND@2" pad="C6"/>
<connect gate="G$1" pin="GND@20" pad="F18"/>
<connect gate="G$1" pin="GND@21" pad="G3"/>
<connect gate="G$1" pin="GND@22" pad="H18"/>
<connect gate="G$1" pin="GND@23" pad="J3"/>
<connect gate="G$1" pin="GND@24" pad="J4"/>
<connect gate="G$1" pin="GND@25" pad="J17"/>
<connect gate="G$1" pin="GND@26" pad="J18"/>
<connect gate="G$1" pin="GND@27" pad="K3"/>
<connect gate="G$1" pin="GND@28" pad="M3"/>
<connect gate="G$1" pin="GND@29" pad="M4"/>
<connect gate="G$1" pin="GND@3" pad="C8"/>
<connect gate="G$1" pin="GND@30" pad="M18"/>
<connect gate="G$1" pin="GND@31" pad="N3"/>
<connect gate="G$1" pin="GND@32" pad="N17"/>
<connect gate="G$1" pin="GND@33" pad="N18"/>
<connect gate="G$1" pin="GND@34" pad="R3"/>
<connect gate="G$1" pin="GND@35" pad="R4"/>
<connect gate="G$1" pin="GND@36" pad="R18"/>
<connect gate="G$1" pin="GND@37" pad="T3"/>
<connect gate="G$1" pin="GND@38" pad="T17"/>
<connect gate="G$1" pin="GND@39" pad="T18"/>
<connect gate="G$1" pin="GND@4" pad="C9"/>
<connect gate="G$1" pin="GND@40" pad="U4"/>
<connect gate="G$1" pin="GND@41" pad="U6"/>
<connect gate="G$1" pin="GND@42" pad="U10"/>
<connect gate="G$1" pin="GND@43" pad="V4"/>
<connect gate="G$1" pin="GND@44" pad="V5"/>
<connect gate="G$1" pin="GND@45" pad="V6"/>
<connect gate="G$1" pin="GND@46" pad="V7"/>
<connect gate="G$1" pin="GND@47" pad="V9"/>
<connect gate="G$1" pin="GND@48" pad="V10"/>
<connect gate="G$1" pin="GND@49" pad="V11"/>
<connect gate="G$1" pin="GND@5" pad="C11"/>
<connect gate="G$1" pin="GND@50" pad="V14"/>
<connect gate="G$1" pin="GND@51" pad="V16"/>
<connect gate="G$1" pin="GND@52" pad="V17"/>
<connect gate="G$1" pin="GND@53" pad="V18"/>
<connect gate="G$1" pin="GND@54" pad="W1"/>
<connect gate="G$1" pin="GND@55" pad="Y1"/>
<connect gate="G$1" pin="GND@56" pad="Y18"/>
<connect gate="G$1" pin="GND@57" pad="Y19"/>
<connect gate="G$1" pin="GND@6" pad="C12"/>
<connect gate="G$1" pin="GND@7" pad="C14"/>
<connect gate="G$1" pin="GND@8" pad="C15"/>
<connect gate="G$1" pin="GND@9" pad="D3"/>
<connect gate="G$1" pin="ID0" pad="K19"/>
<connect gate="G$1" pin="ID1" pad="J19"/>
<connect gate="G$1" pin="ID2" pad="F19"/>
<connect gate="G$1" pin="IOVDD@0" pad="C4"/>
<connect gate="G$1" pin="IOVDD@1" pad="D4"/>
<connect gate="G$1" pin="IOVDD@10" pad="K4"/>
<connect gate="G$1" pin="IOVDD@11" pad="M17"/>
<connect gate="G$1" pin="IOVDD@12" pad="N4"/>
<connect gate="G$1" pin="IOVDD@13" pad="R17"/>
<connect gate="G$1" pin="IOVDD@14" pad="T4"/>
<connect gate="G$1" pin="IOVDD@15" pad="U5"/>
<connect gate="G$1" pin="IOVDD@16" pad="U7"/>
<connect gate="G$1" pin="IOVDD@17" pad="U9"/>
<connect gate="G$1" pin="IOVDD@18" pad="U11"/>
<connect gate="G$1" pin="IOVDD@19" pad="U13"/>
<connect gate="G$1" pin="IOVDD@2" pad="D6"/>
<connect gate="G$1" pin="IOVDD@20" pad="U14"/>
<connect gate="G$1" pin="IOVDD@21" pad="U16"/>
<connect gate="G$1" pin="IOVDD@22" pad="V13"/>
<connect gate="G$1" pin="IOVDD@3" pad="D9"/>
<connect gate="G$1" pin="IOVDD@4" pad="D12"/>
<connect gate="G$1" pin="IOVDD@5" pad="D15"/>
<connect gate="G$1" pin="IOVDD@6" pad="D17"/>
<connect gate="G$1" pin="IOVDD@7" pad="F17"/>
<connect gate="G$1" pin="IOVDD@8" pad="G4"/>
<connect gate="G$1" pin="IOVDD@9" pad="H17"/>
<connect gate="G$1" pin="MS0_B" pad="U1"/>
<connect gate="G$1" pin="MS1_B" pad="U2"/>
<connect gate="G$1" pin="NC0" pad="A1"/>
<connect gate="G$1" pin="NC1" pad="A19"/>
<connect gate="G$1" pin="NC2" pad="A20"/>
<connect gate="G$1" pin="NC3" pad="B20"/>
<connect gate="G$1" pin="NC4" pad="W20"/>
<connect gate="G$1" pin="NC5" pad="Y2"/>
<connect gate="G$1" pin="NC6" pad="Y3"/>
<connect gate="G$1" pin="NC7" pad="Y9"/>
<connect gate="G$1" pin="NC8" pad="Y10"/>
<connect gate="G$1" pin="NC9" pad="Y20"/>
<connect gate="G$1" pin="RD_B" pad="N1"/>
<connect gate="G$1" pin="RESET_B" pad="B16"/>
<connect gate="G$1" pin="RPBA" pad="C20"/>
<connect gate="G$1" pin="SDA10" pad="P1"/>
<connect gate="G$1" pin="SDCAS_B" pad="T2"/>
<connect gate="G$1" pin="SDCKE" pad="T1"/>
<connect gate="G$1" pin="SDCLK0" pad="N2"/>
<connect gate="G$1" pin="SDCLK1" pad="B2"/>
<connect gate="G$1" pin="SDRAS_B" pad="R2"/>
<connect gate="G$1" pin="SDWE_B" pad="R1"/>
<connect gate="G$1" pin="TCK" pad="B4"/>
<connect gate="G$1" pin="TDI" pad="A2"/>
<connect gate="G$1" pin="TDO" pad="B7"/>
<connect gate="G$1" pin="TMS" pad="A3"/>
<connect gate="G$1" pin="TRST" pad="B3"/>
<connect gate="G$1" pin="VDD@0" pad="C7"/>
<connect gate="G$1" pin="VDD@1" pad="C10"/>
<connect gate="G$1" pin="VDD@10" pad="E4"/>
<connect gate="G$1" pin="VDD@11" pad="G17"/>
<connect gate="G$1" pin="VDD@12" pad="G18"/>
<connect gate="G$1" pin="VDD@13" pad="H3"/>
<connect gate="G$1" pin="VDD@14" pad="H4"/>
<connect gate="G$1" pin="VDD@15" pad="K17"/>
<connect gate="G$1" pin="VDD@16" pad="K18"/>
<connect gate="G$1" pin="VDD@17" pad="L3"/>
<connect gate="G$1" pin="VDD@18" pad="L4"/>
<connect gate="G$1" pin="VDD@19" pad="L17"/>
<connect gate="G$1" pin="VDD@2" pad="C13"/>
<connect gate="G$1" pin="VDD@20" pad="L18"/>
<connect gate="G$1" pin="VDD@21" pad="P3"/>
<connect gate="G$1" pin="VDD@22" pad="P4"/>
<connect gate="G$1" pin="VDD@23" pad="P17"/>
<connect gate="G$1" pin="VDD@24" pad="P18"/>
<connect gate="G$1" pin="VDD@25" pad="U3"/>
<connect gate="G$1" pin="VDD@26" pad="U8"/>
<connect gate="G$1" pin="VDD@27" pad="U12"/>
<connect gate="G$1" pin="VDD@28" pad="U15"/>
<connect gate="G$1" pin="VDD@29" pad="U17"/>
<connect gate="G$1" pin="VDD@3" pad="C16"/>
<connect gate="G$1" pin="VDD@30" pad="U18"/>
<connect gate="G$1" pin="VDD@31" pad="V3"/>
<connect gate="G$1" pin="VDD@32" pad="V8"/>
<connect gate="G$1" pin="VDD@33" pad="V12"/>
<connect gate="G$1" pin="VDD@34" pad="V15"/>
<connect gate="G$1" pin="VDD@4" pad="C17"/>
<connect gate="G$1" pin="VDD@5" pad="C18"/>
<connect gate="G$1" pin="VDD@6" pad="D7"/>
<connect gate="G$1" pin="VDD@7" pad="D10"/>
<connect gate="G$1" pin="VDD@8" pad="D13"/>
<connect gate="G$1" pin="VDD@9" pad="E3"/>
<connect gate="G$1" pin="WR_B" pad="P2"/>
<connect gate="G$1" pin="XTAL" pad="Y7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1776206"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_21369" prefix="IC">
<description>&lt;b&gt;SHARC Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: 43623621369_208pinMQFP_bsdl_PrA_0106.txt&lt;br&gt;
http://www.analog.com/static/imported-files/data_sheets/ADSP-21367_21368_21369.pdf</description>
<gates>
<gate name="G$1" symbol="ADSP_21369"/>
</gates>
<devices>
<device name="" package="LQFP208">
<connects>
<connect gate="G$1" pin="ACK" pad="120"/>
<connect gate="G$1" pin="ADDR0" pad="56"/>
<connect gate="G$1" pin="ADDR1" pad="58"/>
<connect gate="G$1" pin="ADDR10" pad="70"/>
<connect gate="G$1" pin="ADDR11" pad="75"/>
<connect gate="G$1" pin="ADDR12" pad="76"/>
<connect gate="G$1" pin="ADDR13" pad="77"/>
<connect gate="G$1" pin="ADDR14" pad="88"/>
<connect gate="G$1" pin="ADDR15" pad="91"/>
<connect gate="G$1" pin="ADDR16" pad="92"/>
<connect gate="G$1" pin="ADDR17" pad="93"/>
<connect gate="G$1" pin="ADDR18" pad="94"/>
<connect gate="G$1" pin="ADDR19" pad="97"/>
<connect gate="G$1" pin="ADDR2" pad="57"/>
<connect gate="G$1" pin="ADDR20" pad="98"/>
<connect gate="G$1" pin="ADDR21" pad="99"/>
<connect gate="G$1" pin="ADDR22" pad="101"/>
<connect gate="G$1" pin="ADDR23" pad="100"/>
<connect gate="G$1" pin="ADDR3" pad="60"/>
<connect gate="G$1" pin="ADDR4" pad="59"/>
<connect gate="G$1" pin="ADDR5" pad="61"/>
<connect gate="G$1" pin="ADDR6" pad="66"/>
<connect gate="G$1" pin="ADDR7" pad="67"/>
<connect gate="G$1" pin="ADDR8" pad="68"/>
<connect gate="G$1" pin="ADDR9" pad="69"/>
<connect gate="G$1" pin="AVDD" pad="81"/>
<connect gate="G$1" pin="AVSS" pad="80"/>
<connect gate="G$1" pin="BOOTCFG0" pad="170"/>
<connect gate="G$1" pin="BOOTCFG1" pad="173"/>
<connect gate="G$1" pin="CLKIN" pad="83"/>
<connect gate="G$1" pin="CLKOUT" pad="201"/>
<connect gate="G$1" pin="CLK_CFG0" pad="169"/>
<connect gate="G$1" pin="CLK_CFG1" pad="171"/>
<connect gate="G$1" pin="DAI1" pad="178"/>
<connect gate="G$1" pin="DAI10" pad="144"/>
<connect gate="G$1" pin="DAI11" pad="143"/>
<connect gate="G$1" pin="DAI12" pad="137"/>
<connect gate="G$1" pin="DAI13" pad="136"/>
<connect gate="G$1" pin="DAI14" pad="135"/>
<connect gate="G$1" pin="DAI15" pad="134"/>
<connect gate="G$1" pin="DAI16" pad="133"/>
<connect gate="G$1" pin="DAI17" pad="132"/>
<connect gate="G$1" pin="DAI18" pad="131"/>
<connect gate="G$1" pin="DAI19" pad="130"/>
<connect gate="G$1" pin="DAI2" pad="176"/>
<connect gate="G$1" pin="DAI20" pad="125"/>
<connect gate="G$1" pin="DAI3" pad="177"/>
<connect gate="G$1" pin="DAI4" pad="175"/>
<connect gate="G$1" pin="DAI5" pad="149"/>
<connect gate="G$1" pin="DAI6" pad="147"/>
<connect gate="G$1" pin="DAI7" pad="148"/>
<connect gate="G$1" pin="DAI8" pad="145"/>
<connect gate="G$1" pin="DAI9" pad="146"/>
<connect gate="G$1" pin="DATA0" pad="48"/>
<connect gate="G$1" pin="DATA1" pad="49"/>
<connect gate="G$1" pin="DATA10" pad="36"/>
<connect gate="G$1" pin="DATA11" pad="35"/>
<connect gate="G$1" pin="DATA12" pad="30"/>
<connect gate="G$1" pin="DATA13" pad="29"/>
<connect gate="G$1" pin="DATA14" pad="28"/>
<connect gate="G$1" pin="DATA15" pad="27"/>
<connect gate="G$1" pin="DATA16" pad="26"/>
<connect gate="G$1" pin="DATA17" pad="21"/>
<connect gate="G$1" pin="DATA18" pad="18"/>
<connect gate="G$1" pin="DATA19" pad="17"/>
<connect gate="G$1" pin="DATA2" pad="46"/>
<connect gate="G$1" pin="DATA20" pad="14"/>
<connect gate="G$1" pin="DATA21" pad="13"/>
<connect gate="G$1" pin="DATA22" pad="12"/>
<connect gate="G$1" pin="DATA23" pad="9"/>
<connect gate="G$1" pin="DATA24" pad="8"/>
<connect gate="G$1" pin="DATA25" pad="7"/>
<connect gate="G$1" pin="DATA26" pad="6"/>
<connect gate="G$1" pin="DATA27" pad="3"/>
<connect gate="G$1" pin="DATA28" pad="2"/>
<connect gate="G$1" pin="DATA29" pad="207"/>
<connect gate="G$1" pin="DATA3" pad="47"/>
<connect gate="G$1" pin="DATA30" pad="205"/>
<connect gate="G$1" pin="DATA31" pad="206"/>
<connect gate="G$1" pin="DATA4" pad="44"/>
<connect gate="G$1" pin="DATA5" pad="45"/>
<connect gate="G$1" pin="DATA6" pad="40"/>
<connect gate="G$1" pin="DATA7" pad="39"/>
<connect gate="G$1" pin="DATA8" pad="38"/>
<connect gate="G$1" pin="DATA9" pad="37"/>
<connect gate="G$1" pin="DPI1" pad="199"/>
<connect gate="G$1" pin="DPI10" pad="187"/>
<connect gate="G$1" pin="DPI11" pad="186"/>
<connect gate="G$1" pin="DPI12" pad="185"/>
<connect gate="G$1" pin="DPI13" pad="184"/>
<connect gate="G$1" pin="DPI14" pad="183"/>
<connect gate="G$1" pin="DPI2" pad="200"/>
<connect gate="G$1" pin="DPI3" pad="198"/>
<connect gate="G$1" pin="DPI4" pad="197"/>
<connect gate="G$1" pin="DPI5" pad="196"/>
<connect gate="G$1" pin="DPI6" pad="195"/>
<connect gate="G$1" pin="DPI7" pad="190"/>
<connect gate="G$1" pin="DPI8" pad="189"/>
<connect gate="G$1" pin="DPI9" pad="188"/>
<connect gate="G$1" pin="EMU_B" pad="172"/>
<connect gate="G$1" pin="FLAG0" pad="124"/>
<connect gate="G$1" pin="FLAG1" pad="123"/>
<connect gate="G$1" pin="FLAG2" pad="122"/>
<connect gate="G$1" pin="FLAG3" pad="121"/>
<connect gate="G$1" pin="GND@0" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@10" pad="54"/>
<connect gate="G$1" pin="GND@11" pad="62"/>
<connect gate="G$1" pin="GND@12" pad="64"/>
<connect gate="G$1" pin="GND@13" pad="71"/>
<connect gate="G$1" pin="GND@14" pad="73"/>
<connect gate="G$1" pin="GND@15" pad="78"/>
<connect gate="G$1" pin="GND@16" pad="82"/>
<connect gate="G$1" pin="GND@17" pad="86"/>
<connect gate="G$1" pin="GND@18" pad="89"/>
<connect gate="G$1" pin="GND@19" pad="95"/>
<connect gate="G$1" pin="GND@2" pad="16"/>
<connect gate="G$1" pin="GND@20" pad="106"/>
<connect gate="G$1" pin="GND@21" pad="114"/>
<connect gate="G$1" pin="GND@22" pad="117"/>
<connect gate="G$1" pin="GND@23" pad="126"/>
<connect gate="G$1" pin="GND@24" pad="128"/>
<connect gate="G$1" pin="GND@25" pad="140"/>
<connect gate="G$1" pin="GND@26" pad="142"/>
<connect gate="G$1" pin="GND@27" pad="151"/>
<connect gate="G$1" pin="GND@28" pad="153"/>
<connect gate="G$1" pin="GND@29" pad="155"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="GND@30" pad="159"/>
<connect gate="G$1" pin="GND@31" pad="166"/>
<connect gate="G$1" pin="GND@32" pad="180"/>
<connect gate="G$1" pin="GND@33" pad="182"/>
<connect gate="G$1" pin="GND@34" pad="192"/>
<connect gate="G$1" pin="GND@35" pad="194"/>
<connect gate="G$1" pin="GND@36" pad="204"/>
<connect gate="G$1" pin="GND@4" pad="23"/>
<connect gate="G$1" pin="GND@5" pad="25"/>
<connect gate="G$1" pin="GND@6" pad="32"/>
<connect gate="G$1" pin="GND@7" pad="34"/>
<connect gate="G$1" pin="GND@8" pad="42"/>
<connect gate="G$1" pin="GND@9" pad="51"/>
<connect gate="G$1" pin="IOVDD@0" pad="5"/>
<connect gate="G$1" pin="IOVDD@1" pad="15"/>
<connect gate="G$1" pin="IOVDD@10" pad="96"/>
<connect gate="G$1" pin="IOVDD@11" pad="107"/>
<connect gate="G$1" pin="IOVDD@12" pad="115"/>
<connect gate="G$1" pin="IOVDD@13" pad="129"/>
<connect gate="G$1" pin="IOVDD@14" pad="139"/>
<connect gate="G$1" pin="IOVDD@15" pad="150"/>
<connect gate="G$1" pin="IOVDD@16" pad="179"/>
<connect gate="G$1" pin="IOVDD@17" pad="191"/>
<connect gate="G$1" pin="IOVDD@18" pad="203"/>
<connect gate="G$1" pin="IOVDD@2" pad="31"/>
<connect gate="G$1" pin="IOVDD@3" pad="41"/>
<connect gate="G$1" pin="IOVDD@4" pad="50"/>
<connect gate="G$1" pin="IOVDD@5" pad="55"/>
<connect gate="G$1" pin="IOVDD@6" pad="65"/>
<connect gate="G$1" pin="IOVDD@7" pad="74"/>
<connect gate="G$1" pin="IOVDD@8" pad="85"/>
<connect gate="G$1" pin="IOVDD@9" pad="90"/>
<connect gate="G$1" pin="MS0_B" pad="103"/>
<connect gate="G$1" pin="MS1_B" pad="102"/>
<connect gate="G$1" pin="RD_B" pad="119"/>
<connect gate="G$1" pin="RESET_B" pad="202"/>
<connect gate="G$1" pin="SDA10" pad="113"/>
<connect gate="G$1" pin="SDCAS_B" pad="108"/>
<connect gate="G$1" pin="SDCKE" pad="110"/>
<connect gate="G$1" pin="SDCLK0" pad="116"/>
<connect gate="G$1" pin="SDRAS_B" pad="109"/>
<connect gate="G$1" pin="SDWE_B" pad="111"/>
<connect gate="G$1" pin="TCK" pad="165"/>
<connect gate="G$1" pin="TDI" pad="163"/>
<connect gate="G$1" pin="TDO" pad="174"/>
<connect gate="G$1" pin="TMS" pad="168"/>
<connect gate="G$1" pin="TRST" pad="164"/>
<connect gate="G$1" pin="VDD@0" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="11"/>
<connect gate="G$1" pin="VDD@10" pad="72"/>
<connect gate="G$1" pin="VDD@11" pad="79"/>
<connect gate="G$1" pin="VDD@12" pad="87"/>
<connect gate="G$1" pin="VDD@13" pad="104"/>
<connect gate="G$1" pin="VDD@14" pad="105"/>
<connect gate="G$1" pin="VDD@15" pad="118"/>
<connect gate="G$1" pin="VDD@16" pad="127"/>
<connect gate="G$1" pin="VDD@17" pad="138"/>
<connect gate="G$1" pin="VDD@18" pad="141"/>
<connect gate="G$1" pin="VDD@19" pad="152"/>
<connect gate="G$1" pin="VDD@2" pad="19"/>
<connect gate="G$1" pin="VDD@20" pad="154"/>
<connect gate="G$1" pin="VDD@21" pad="156"/>
<connect gate="G$1" pin="VDD@22" pad="157"/>
<connect gate="G$1" pin="VDD@23" pad="158"/>
<connect gate="G$1" pin="VDD@24" pad="160"/>
<connect gate="G$1" pin="VDD@25" pad="161"/>
<connect gate="G$1" pin="VDD@26" pad="162"/>
<connect gate="G$1" pin="VDD@27" pad="167"/>
<connect gate="G$1" pin="VDD@28" pad="181"/>
<connect gate="G$1" pin="VDD@29" pad="193"/>
<connect gate="G$1" pin="VDD@3" pad="22"/>
<connect gate="G$1" pin="VDD@30" pad="208"/>
<connect gate="G$1" pin="VDD@4" pad="24"/>
<connect gate="G$1" pin="VDD@5" pad="33"/>
<connect gate="G$1" pin="VDD@6" pad="43"/>
<connect gate="G$1" pin="VDD@7" pad="52"/>
<connect gate="G$1" pin="VDD@8" pad="53"/>
<connect gate="G$1" pin="VDD@9" pad="63"/>
<connect gate="G$1" pin="WR_B" pad="112"/>
<connect gate="G$1" pin="XTAL" pad="84"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_21375" prefix="IC">
<description>&lt;b&gt;SHARC Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: 816925549AD21375_2A7CB107_4651_47A7_9AAE_75132EECEAE5_bsdl.txt</description>
<gates>
<gate name="G$1" symbol="ADSP_21375"/>
</gates>
<devices>
<device name="" package="LQFP208">
<connects>
<connect gate="G$1" pin="ACK" pad="120"/>
<connect gate="G$1" pin="ADDR0" pad="56"/>
<connect gate="G$1" pin="ADDR1" pad="58"/>
<connect gate="G$1" pin="ADDR10" pad="70"/>
<connect gate="G$1" pin="ADDR11" pad="75"/>
<connect gate="G$1" pin="ADDR12" pad="76"/>
<connect gate="G$1" pin="ADDR13" pad="77"/>
<connect gate="G$1" pin="ADDR14" pad="88"/>
<connect gate="G$1" pin="ADDR15" pad="91"/>
<connect gate="G$1" pin="ADDR16" pad="92"/>
<connect gate="G$1" pin="ADDR17" pad="93"/>
<connect gate="G$1" pin="ADDR18" pad="94"/>
<connect gate="G$1" pin="ADDR19" pad="97"/>
<connect gate="G$1" pin="ADDR2" pad="57"/>
<connect gate="G$1" pin="ADDR20" pad="98"/>
<connect gate="G$1" pin="ADDR21" pad="99"/>
<connect gate="G$1" pin="ADDR22" pad="101"/>
<connect gate="G$1" pin="ADDR23" pad="100"/>
<connect gate="G$1" pin="ADDR3" pad="60"/>
<connect gate="G$1" pin="ADDR4" pad="59"/>
<connect gate="G$1" pin="ADDR5" pad="61"/>
<connect gate="G$1" pin="ADDR6" pad="66"/>
<connect gate="G$1" pin="ADDR7" pad="67"/>
<connect gate="G$1" pin="ADDR8" pad="68"/>
<connect gate="G$1" pin="ADDR9" pad="69"/>
<connect gate="G$1" pin="BOOTCFG0" pad="170"/>
<connect gate="G$1" pin="BOOTCFG1" pad="173"/>
<connect gate="G$1" pin="CLKIN" pad="83"/>
<connect gate="G$1" pin="CLKOUT" pad="201"/>
<connect gate="G$1" pin="CLK_CFG0" pad="169"/>
<connect gate="G$1" pin="CLK_CFG1" pad="171"/>
<connect gate="G$1" pin="DAI1" pad="178"/>
<connect gate="G$1" pin="DAI10" pad="144"/>
<connect gate="G$1" pin="DAI11" pad="143"/>
<connect gate="G$1" pin="DAI12" pad="137"/>
<connect gate="G$1" pin="DAI13" pad="136"/>
<connect gate="G$1" pin="DAI14" pad="135"/>
<connect gate="G$1" pin="DAI15" pad="134"/>
<connect gate="G$1" pin="DAI16" pad="133"/>
<connect gate="G$1" pin="DAI17" pad="132"/>
<connect gate="G$1" pin="DAI18" pad="131"/>
<connect gate="G$1" pin="DAI19" pad="130"/>
<connect gate="G$1" pin="DAI2" pad="176"/>
<connect gate="G$1" pin="DAI20" pad="125"/>
<connect gate="G$1" pin="DAI3" pad="177"/>
<connect gate="G$1" pin="DAI4" pad="175"/>
<connect gate="G$1" pin="DAI5" pad="149"/>
<connect gate="G$1" pin="DAI6" pad="147"/>
<connect gate="G$1" pin="DAI7" pad="148"/>
<connect gate="G$1" pin="DAI8" pad="145"/>
<connect gate="G$1" pin="DAI9" pad="146"/>
<connect gate="G$1" pin="DATA0" pad="48"/>
<connect gate="G$1" pin="DATA1" pad="49"/>
<connect gate="G$1" pin="DATA10" pad="36"/>
<connect gate="G$1" pin="DATA11" pad="35"/>
<connect gate="G$1" pin="DATA12" pad="30"/>
<connect gate="G$1" pin="DATA13" pad="29"/>
<connect gate="G$1" pin="DATA14" pad="28"/>
<connect gate="G$1" pin="DATA15" pad="27"/>
<connect gate="G$1" pin="DATA2" pad="46"/>
<connect gate="G$1" pin="DATA3" pad="47"/>
<connect gate="G$1" pin="DATA4" pad="44"/>
<connect gate="G$1" pin="DATA5" pad="45"/>
<connect gate="G$1" pin="DATA6" pad="40"/>
<connect gate="G$1" pin="DATA7" pad="39"/>
<connect gate="G$1" pin="DATA8" pad="38"/>
<connect gate="G$1" pin="DATA9" pad="37"/>
<connect gate="G$1" pin="DPI1" pad="199"/>
<connect gate="G$1" pin="DPI10" pad="187"/>
<connect gate="G$1" pin="DPI11" pad="186"/>
<connect gate="G$1" pin="DPI12" pad="185"/>
<connect gate="G$1" pin="DPI13" pad="184"/>
<connect gate="G$1" pin="DPI14" pad="183"/>
<connect gate="G$1" pin="DPI2" pad="200"/>
<connect gate="G$1" pin="DPI3" pad="198"/>
<connect gate="G$1" pin="DPI4" pad="197"/>
<connect gate="G$1" pin="DPI5" pad="196"/>
<connect gate="G$1" pin="DPI6" pad="195"/>
<connect gate="G$1" pin="DPI7" pad="190"/>
<connect gate="G$1" pin="DPI8" pad="189"/>
<connect gate="G$1" pin="DPI9" pad="188"/>
<connect gate="G$1" pin="EMU" pad="172"/>
<connect gate="G$1" pin="FLAG0" pad="124"/>
<connect gate="G$1" pin="FLAG1" pad="123"/>
<connect gate="G$1" pin="FLAG2" pad="122"/>
<connect gate="G$1" pin="FLAG3" pad="121"/>
<connect gate="G$1" pin="GND@0" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@10" pad="64"/>
<connect gate="G$1" pin="GND@11" pad="71"/>
<connect gate="G$1" pin="GND@12" pad="73"/>
<connect gate="G$1" pin="GND@13" pad="78"/>
<connect gate="G$1" pin="GND@14" pad="82"/>
<connect gate="G$1" pin="GND@15" pad="86"/>
<connect gate="G$1" pin="GND@16" pad="89"/>
<connect gate="G$1" pin="GND@17" pad="95"/>
<connect gate="G$1" pin="GND@18" pad="106"/>
<connect gate="G$1" pin="GND@19" pad="114"/>
<connect gate="G$1" pin="GND@2" pad="23"/>
<connect gate="G$1" pin="GND@20" pad="117"/>
<connect gate="G$1" pin="GND@21" pad="126"/>
<connect gate="G$1" pin="GND@22" pad="128"/>
<connect gate="G$1" pin="GND@23" pad="140"/>
<connect gate="G$1" pin="GND@24" pad="142"/>
<connect gate="G$1" pin="GND@25" pad="151"/>
<connect gate="G$1" pin="GND@26" pad="153"/>
<connect gate="G$1" pin="GND@27" pad="155"/>
<connect gate="G$1" pin="GND@28" pad="159"/>
<connect gate="G$1" pin="GND@29" pad="166"/>
<connect gate="G$1" pin="GND@3" pad="25"/>
<connect gate="G$1" pin="GND@30" pad="180"/>
<connect gate="G$1" pin="GND@31" pad="182"/>
<connect gate="G$1" pin="GND@32" pad="192"/>
<connect gate="G$1" pin="GND@33" pad="194"/>
<connect gate="G$1" pin="GND@34" pad="204"/>
<connect gate="G$1" pin="GND@4" pad="32"/>
<connect gate="G$1" pin="GND@5" pad="34"/>
<connect gate="G$1" pin="GND@6" pad="42"/>
<connect gate="G$1" pin="GND@7" pad="51"/>
<connect gate="G$1" pin="GND@8" pad="54"/>
<connect gate="G$1" pin="GND@9" pad="62"/>
<connect gate="G$1" pin="IOVDD@0" pad="5"/>
<connect gate="G$1" pin="IOVDD@1" pad="31"/>
<connect gate="G$1" pin="IOVDD@10" pad="107"/>
<connect gate="G$1" pin="IOVDD@11" pad="115"/>
<connect gate="G$1" pin="IOVDD@12" pad="129"/>
<connect gate="G$1" pin="IOVDD@13" pad="139"/>
<connect gate="G$1" pin="IOVDD@14" pad="150"/>
<connect gate="G$1" pin="IOVDD@15" pad="179"/>
<connect gate="G$1" pin="IOVDD@16" pad="191"/>
<connect gate="G$1" pin="IOVDD@17" pad="203"/>
<connect gate="G$1" pin="IOVDD@2" pad="41"/>
<connect gate="G$1" pin="IOVDD@3" pad="50"/>
<connect gate="G$1" pin="IOVDD@4" pad="55"/>
<connect gate="G$1" pin="IOVDD@5" pad="65"/>
<connect gate="G$1" pin="IOVDD@6" pad="74"/>
<connect gate="G$1" pin="IOVDD@7" pad="85"/>
<connect gate="G$1" pin="IOVDD@8" pad="90"/>
<connect gate="G$1" pin="IOVDD@9" pad="96"/>
<connect gate="G$1" pin="MS0" pad="103"/>
<connect gate="G$1" pin="MS1" pad="102"/>
<connect gate="G$1" pin="NC0" pad="2"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC10" pad="16"/>
<connect gate="G$1" pin="NC11" pad="17"/>
<connect gate="G$1" pin="NC12" pad="18"/>
<connect gate="G$1" pin="NC13" pad="19"/>
<connect gate="G$1" pin="NC14" pad="20"/>
<connect gate="G$1" pin="NC15" pad="21"/>
<connect gate="G$1" pin="NC16" pad="26"/>
<connect gate="G$1" pin="NC17" pad="80"/>
<connect gate="G$1" pin="NC18" pad="81"/>
<connect gate="G$1" pin="NC19" pad="205"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="NC20" pad="206"/>
<connect gate="G$1" pin="NC21" pad="207"/>
<connect gate="G$1" pin="NC3" pad="7"/>
<connect gate="G$1" pin="NC4" pad="8"/>
<connect gate="G$1" pin="NC5" pad="9"/>
<connect gate="G$1" pin="NC6" pad="12"/>
<connect gate="G$1" pin="NC7" pad="13"/>
<connect gate="G$1" pin="NC8" pad="14"/>
<connect gate="G$1" pin="NC9" pad="15"/>
<connect gate="G$1" pin="RD" pad="119"/>
<connect gate="G$1" pin="RESET" pad="202"/>
<connect gate="G$1" pin="SDA10" pad="113"/>
<connect gate="G$1" pin="SDCAS" pad="108"/>
<connect gate="G$1" pin="SDCKE" pad="110"/>
<connect gate="G$1" pin="SDCLK0" pad="116"/>
<connect gate="G$1" pin="SDRAS" pad="109"/>
<connect gate="G$1" pin="SDWE" pad="111"/>
<connect gate="G$1" pin="TCK" pad="165"/>
<connect gate="G$1" pin="TDI" pad="163"/>
<connect gate="G$1" pin="TDO" pad="174"/>
<connect gate="G$1" pin="TMS" pad="168"/>
<connect gate="G$1" pin="TRST" pad="164"/>
<connect gate="G$1" pin="VDD@0" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="11"/>
<connect gate="G$1" pin="VDD@10" pad="79"/>
<connect gate="G$1" pin="VDD@11" pad="87"/>
<connect gate="G$1" pin="VDD@12" pad="104"/>
<connect gate="G$1" pin="VDD@13" pad="105"/>
<connect gate="G$1" pin="VDD@14" pad="118"/>
<connect gate="G$1" pin="VDD@15" pad="127"/>
<connect gate="G$1" pin="VDD@16" pad="138"/>
<connect gate="G$1" pin="VDD@17" pad="141"/>
<connect gate="G$1" pin="VDD@18" pad="152"/>
<connect gate="G$1" pin="VDD@19" pad="154"/>
<connect gate="G$1" pin="VDD@2" pad="22"/>
<connect gate="G$1" pin="VDD@20" pad="156"/>
<connect gate="G$1" pin="VDD@21" pad="157"/>
<connect gate="G$1" pin="VDD@22" pad="158"/>
<connect gate="G$1" pin="VDD@23" pad="160"/>
<connect gate="G$1" pin="VDD@24" pad="161"/>
<connect gate="G$1" pin="VDD@25" pad="162"/>
<connect gate="G$1" pin="VDD@26" pad="167"/>
<connect gate="G$1" pin="VDD@27" pad="181"/>
<connect gate="G$1" pin="VDD@28" pad="193"/>
<connect gate="G$1" pin="VDD@29" pad="208"/>
<connect gate="G$1" pin="VDD@3" pad="24"/>
<connect gate="G$1" pin="VDD@4" pad="33"/>
<connect gate="G$1" pin="VDD@5" pad="43"/>
<connect gate="G$1" pin="VDD@6" pad="52"/>
<connect gate="G$1" pin="VDD@7" pad="53"/>
<connect gate="G$1" pin="VDD@8" pad="63"/>
<connect gate="G$1" pin="VDD@9" pad="72"/>
<connect gate="G$1" pin="WR" pad="112"/>
<connect gate="G$1" pin="XTAL2" pad="84"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1776212"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_21462W" prefix="IC">
<description>&lt;b&gt;SHARC Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: ADSP_21462W_324_CSPBGA_bsdl.txt&lt;br&gt;
http://www.analog.com/static/imported-files/data_sheets/ADSP_21462W_21465W_21467_21469_21469W.pdf</description>
<gates>
<gate name="G$1" symbol="ADSP_21462W"/>
</gates>
<devices>
<device name="" package="BGA_324_CSP">
<connects>
<connect gate="G$1" pin="AGND" pad="H2"/>
<connect gate="G$1" pin="AMI_ACK" pad="R10"/>
<connect gate="G$1" pin="AMI_ADDR0" pad="V16"/>
<connect gate="G$1" pin="AMI_ADDR01" pad="U16"/>
<connect gate="G$1" pin="AMI_ADDR02" pad="T16"/>
<connect gate="G$1" pin="AMI_ADDR03" pad="R16"/>
<connect gate="G$1" pin="AMI_ADDR04" pad="V15"/>
<connect gate="G$1" pin="AMI_ADDR05" pad="U15"/>
<connect gate="G$1" pin="AMI_ADDR06" pad="T15"/>
<connect gate="G$1" pin="AMI_ADDR07" pad="R15"/>
<connect gate="G$1" pin="AMI_ADDR08" pad="V14"/>
<connect gate="G$1" pin="AMI_ADDR09" pad="U14"/>
<connect gate="G$1" pin="AMI_ADDR10" pad="T14"/>
<connect gate="G$1" pin="AMI_ADDR11" pad="R14"/>
<connect gate="G$1" pin="AMI_ADDR12" pad="V13"/>
<connect gate="G$1" pin="AMI_ADDR13" pad="U13"/>
<connect gate="G$1" pin="AMI_ADDR14" pad="T13"/>
<connect gate="G$1" pin="AMI_ADDR15" pad="R13"/>
<connect gate="G$1" pin="AMI_ADDR16" pad="V12"/>
<connect gate="G$1" pin="AMI_ADDR17" pad="U12"/>
<connect gate="G$1" pin="AMI_ADDR18" pad="T12"/>
<connect gate="G$1" pin="AMI_ADDR19" pad="R12"/>
<connect gate="G$1" pin="AMI_ADDR20" pad="V11"/>
<connect gate="G$1" pin="AMI_ADDR21" pad="U11"/>
<connect gate="G$1" pin="AMI_ADDR22" pad="T11"/>
<connect gate="G$1" pin="AMI_ADDR23" pad="R11"/>
<connect gate="G$1" pin="AMI_DATA0" pad="U18"/>
<connect gate="G$1" pin="AMI_DATA1" pad="T18"/>
<connect gate="G$1" pin="AMI_DATA2" pad="R18"/>
<connect gate="G$1" pin="AMI_DATA3" pad="P18"/>
<connect gate="G$1" pin="AMI_DATA4" pad="V17"/>
<connect gate="G$1" pin="AMI_DATA5" pad="U17"/>
<connect gate="G$1" pin="AMI_DATA6" pad="T17"/>
<connect gate="G$1" pin="AMI_DATA7" pad="R17"/>
<connect gate="G$1" pin="AMI_MS0_B" pad="T10"/>
<connect gate="G$1" pin="AMI_MS1_B" pad="U10"/>
<connect gate="G$1" pin="AMI_RD_B" pad="J4"/>
<connect gate="G$1" pin="AMI_WR_B" pad="V10"/>
<connect gate="G$1" pin="BOOT_CFG0" pad="J2"/>
<connect gate="G$1" pin="BOOT_CFG1" pad="J3"/>
<connect gate="G$1" pin="BOOT_CFG2" pad="H3"/>
<connect gate="G$1" pin="CLKIN" pad="L1"/>
<connect gate="G$1" pin="CLKOUT" pad="M2"/>
<connect gate="G$1" pin="CLK_CFG0" pad="G1"/>
<connect gate="G$1" pin="CLK_CFG1" pad="G2"/>
<connect gate="G$1" pin="DAI_P01" pad="R6"/>
<connect gate="G$1" pin="DAI_P02" pad="V5"/>
<connect gate="G$1" pin="DAI_P03" pad="R7"/>
<connect gate="G$1" pin="DAI_P04" pad="R3"/>
<connect gate="G$1" pin="DAI_P05" pad="U5"/>
<connect gate="G$1" pin="DAI_P06" pad="T5"/>
<connect gate="G$1" pin="DAI_P07" pad="V6"/>
<connect gate="G$1" pin="DAI_P08" pad="V2"/>
<connect gate="G$1" pin="DAI_P09" pad="R5"/>
<connect gate="G$1" pin="DAI_P10" pad="V4"/>
<connect gate="G$1" pin="DAI_P11" pad="U4"/>
<connect gate="G$1" pin="DAI_P12" pad="T4"/>
<connect gate="G$1" pin="DAI_P13" pad="U6"/>
<connect gate="G$1" pin="DAI_P14" pad="U2"/>
<connect gate="G$1" pin="DAI_P15" pad="R4"/>
<connect gate="G$1" pin="DAI_P16" pad="V3"/>
<connect gate="G$1" pin="DAI_P17" pad="U3"/>
<connect gate="G$1" pin="DAI_P18" pad="T3"/>
<connect gate="G$1" pin="DAI_P19" pad="T6"/>
<connect gate="G$1" pin="DAI_P20" pad="T2"/>
<connect gate="G$1" pin="DDR2_ADDR0" pad="D13"/>
<connect gate="G$1" pin="DDR2_ADDR01" pad="C13"/>
<connect gate="G$1" pin="DDR2_ADDR02" pad="D14"/>
<connect gate="G$1" pin="DDR2_ADDR03" pad="C14"/>
<connect gate="G$1" pin="DDR2_ADDR04" pad="B14"/>
<connect gate="G$1" pin="DDR2_ADDR05" pad="A14"/>
<connect gate="G$1" pin="DDR2_ADDR06" pad="D15"/>
<connect gate="G$1" pin="DDR2_ADDR07" pad="C15"/>
<connect gate="G$1" pin="DDR2_ADDR08" pad="B15"/>
<connect gate="G$1" pin="DDR2_ADDR09" pad="A15"/>
<connect gate="G$1" pin="DDR2_ADDR10" pad="D16"/>
<connect gate="G$1" pin="DDR2_ADDR11" pad="C16"/>
<connect gate="G$1" pin="DDR2_ADDR12" pad="B16"/>
<connect gate="G$1" pin="DDR2_ADDR13" pad="A16"/>
<connect gate="G$1" pin="DDR2_ADDR14" pad="B17"/>
<connect gate="G$1" pin="DDR2_ADDR15" pad="A17"/>
<connect gate="G$1" pin="DDR2_BA0" pad="C18"/>
<connect gate="G$1" pin="DDR2_BA1" pad="C17"/>
<connect gate="G$1" pin="DDR2_BA2" pad="B18"/>
<connect gate="G$1" pin="DDR2_CAS_B" pad="C7"/>
<connect gate="G$1" pin="DDR2_CKE" pad="E1"/>
<connect gate="G$1" pin="DDR2_CLK0" pad="B7"/>
<connect gate="G$1" pin="DDR2_CLK0_B" pad="A7"/>
<connect gate="G$1" pin="DDR2_CLK1" pad="B13"/>
<connect gate="G$1" pin="DDR2_CLK1_B" pad="A13"/>
<connect gate="G$1" pin="DDR2_CS0_B" pad="C1"/>
<connect gate="G$1" pin="DDR2_CS1_B" pad="D1"/>
<connect gate="G$1" pin="DDR2_CS2_B" pad="C2"/>
<connect gate="G$1" pin="DDR2_CS3_B" pad="D2"/>
<connect gate="G$1" pin="DDR2_DATA0" pad="B2"/>
<connect gate="G$1" pin="DDR2_DATA01" pad="A2"/>
<connect gate="G$1" pin="DDR2_DATA02" pad="B3"/>
<connect gate="G$1" pin="DDR2_DATA03" pad="A3"/>
<connect gate="G$1" pin="DDR2_DATA04" pad="B5"/>
<connect gate="G$1" pin="DDR2_DATA05" pad="A5"/>
<connect gate="G$1" pin="DDR2_DATA06" pad="B6"/>
<connect gate="G$1" pin="DDR2_DATA07" pad="A6"/>
<connect gate="G$1" pin="DDR2_DATA08" pad="B8"/>
<connect gate="G$1" pin="DDR2_DATA09" pad="A8"/>
<connect gate="G$1" pin="DDR2_DATA10" pad="B9"/>
<connect gate="G$1" pin="DDR2_DATA11" pad="A9"/>
<connect gate="G$1" pin="DDR2_DATA12" pad="A11"/>
<connect gate="G$1" pin="DDR2_DATA13" pad="B11"/>
<connect gate="G$1" pin="DDR2_DATA14" pad="A12"/>
<connect gate="G$1" pin="DDR2_DATA15" pad="B12"/>
<connect gate="G$1" pin="DDR2_DM0" pad="C3"/>
<connect gate="G$1" pin="DDR2_DM1" pad="C11"/>
<connect gate="G$1" pin="DDR2_DQS0" pad="A4"/>
<connect gate="G$1" pin="DDR2_DQS0_B" pad="B4"/>
<connect gate="G$1" pin="DDR2_DQS1" pad="A10"/>
<connect gate="G$1" pin="DDR2_DQS1_B" pad="B10"/>
<connect gate="G$1" pin="DDR2_ODT" pad="B1"/>
<connect gate="G$1" pin="DDR2_RAS_B" pad="C9"/>
<connect gate="G$1" pin="DDR2_WE_B" pad="C10"/>
<connect gate="G$1" pin="DPI_P01" pad="R2"/>
<connect gate="G$1" pin="DPI_P02" pad="U1"/>
<connect gate="G$1" pin="DPI_P03" pad="T1"/>
<connect gate="G$1" pin="DPI_P04" pad="R1"/>
<connect gate="G$1" pin="DPI_P05" pad="P1"/>
<connect gate="G$1" pin="DPI_P06" pad="P2"/>
<connect gate="G$1" pin="DPI_P07" pad="P3"/>
<connect gate="G$1" pin="DPI_P08" pad="P4"/>
<connect gate="G$1" pin="DPI_P09" pad="N1"/>
<connect gate="G$1" pin="DPI_P10" pad="N2"/>
<connect gate="G$1" pin="DPI_P11" pad="N3"/>
<connect gate="G$1" pin="DPI_P12" pad="N4"/>
<connect gate="G$1" pin="DPI_P13" pad="M3"/>
<connect gate="G$1" pin="DPI_P14" pad="M4"/>
<connect gate="G$1" pin="EMU_B" pad="K2"/>
<connect gate="G$1" pin="FLAG0" pad="R8"/>
<connect gate="G$1" pin="FLAG1" pad="V7"/>
<connect gate="G$1" pin="FLAG2" pad="U7"/>
<connect gate="G$1" pin="FLAG3" pad="T7"/>
<connect gate="G$1" pin="GND@0" pad="A1"/>
<connect gate="G$1" pin="GND@1" pad="A18"/>
<connect gate="G$1" pin="GND@10" pad="E3"/>
<connect gate="G$1" pin="GND@11" pad="E5"/>
<connect gate="G$1" pin="GND@12" pad="E12"/>
<connect gate="G$1" pin="GND@13" pad="E13"/>
<connect gate="G$1" pin="GND@14" pad="E16"/>
<connect gate="G$1" pin="GND@15" pad="F1"/>
<connect gate="G$1" pin="GND@16" pad="F2"/>
<connect gate="G$1" pin="GND@17" pad="F4"/>
<connect gate="G$1" pin="GND@18" pad="F14"/>
<connect gate="G$1" pin="GND@19" pad="F16"/>
<connect gate="G$1" pin="GND@2" pad="C4"/>
<connect gate="G$1" pin="GND@20" pad="G3"/>
<connect gate="G$1" pin="GND@21" pad="G4"/>
<connect gate="G$1" pin="GND@22" pad="G5"/>
<connect gate="G$1" pin="GND@23" pad="G7"/>
<connect gate="G$1" pin="GND@24" pad="G8"/>
<connect gate="G$1" pin="GND@25" pad="G9"/>
<connect gate="G$1" pin="GND@26" pad="G10"/>
<connect gate="G$1" pin="GND@27" pad="G11"/>
<connect gate="G$1" pin="GND@28" pad="G12"/>
<connect gate="G$1" pin="GND@29" pad="G15"/>
<connect gate="G$1" pin="GND@3" pad="C6"/>
<connect gate="G$1" pin="GND@30" pad="H4"/>
<connect gate="G$1" pin="GND@31" pad="H7"/>
<connect gate="G$1" pin="GND@32" pad="H8"/>
<connect gate="G$1" pin="GND@33" pad="H9"/>
<connect gate="G$1" pin="GND@34" pad="H10"/>
<connect gate="G$1" pin="GND@35" pad="H11"/>
<connect gate="G$1" pin="GND@36" pad="H12"/>
<connect gate="G$1" pin="GND@37" pad="J1"/>
<connect gate="G$1" pin="GND@38" pad="J7"/>
<connect gate="G$1" pin="GND@39" pad="J8"/>
<connect gate="G$1" pin="GND@4" pad="C8"/>
<connect gate="G$1" pin="GND@40" pad="J9"/>
<connect gate="G$1" pin="GND@41" pad="J10"/>
<connect gate="G$1" pin="GND@42" pad="J11"/>
<connect gate="G$1" pin="GND@43" pad="J12"/>
<connect gate="G$1" pin="GND@44" pad="J14"/>
<connect gate="G$1" pin="GND@45" pad="J17"/>
<connect gate="G$1" pin="GND@46" pad="K5"/>
<connect gate="G$1" pin="GND@47" pad="K7"/>
<connect gate="G$1" pin="GND@48" pad="K8"/>
<connect gate="G$1" pin="GND@49" pad="K9"/>
<connect gate="G$1" pin="GND@5" pad="D5"/>
<connect gate="G$1" pin="GND@50" pad="K10"/>
<connect gate="G$1" pin="GND@51" pad="K11"/>
<connect gate="G$1" pin="GND@52" pad="K12"/>
<connect gate="G$1" pin="GND@53" pad="L7"/>
<connect gate="G$1" pin="GND@54" pad="L8"/>
<connect gate="G$1" pin="GND@55" pad="L9"/>
<connect gate="G$1" pin="GND@56" pad="L10"/>
<connect gate="G$1" pin="GND@57" pad="L11"/>
<connect gate="G$1" pin="GND@58" pad="L12"/>
<connect gate="G$1" pin="GND@59" pad="L14"/>
<connect gate="G$1" pin="GND@6" pad="D7"/>
<connect gate="G$1" pin="GND@60" pad="M5"/>
<connect gate="G$1" pin="GND@61" pad="M7"/>
<connect gate="G$1" pin="GND@62" pad="M8"/>
<connect gate="G$1" pin="GND@63" pad="M9"/>
<connect gate="G$1" pin="GND@64" pad="M10"/>
<connect gate="G$1" pin="GND@65" pad="M11"/>
<connect gate="G$1" pin="GND@66" pad="M12"/>
<connect gate="G$1" pin="GND@67" pad="N14"/>
<connect gate="G$1" pin="GND@68" pad="N17"/>
<connect gate="G$1" pin="GND@69" pad="P5"/>
<connect gate="G$1" pin="GND@7" pad="D9"/>
<connect gate="G$1" pin="GND@70" pad="P7"/>
<connect gate="G$1" pin="GND@71" pad="P9"/>
<connect gate="G$1" pin="GND@72" pad="P11"/>
<connect gate="G$1" pin="GND@73" pad="P13"/>
<connect gate="G$1" pin="GND@74" pad="R9"/>
<connect gate="G$1" pin="GND@75" pad="V1"/>
<connect gate="G$1" pin="GND@76" pad="V18"/>
<connect gate="G$1" pin="GND@8" pad="D10"/>
<connect gate="G$1" pin="GND@9" pad="D17"/>
<connect gate="G$1" pin="LACK_0" pad="K17"/>
<connect gate="G$1" pin="LACK_1" pad="P17"/>
<connect gate="G$1" pin="LCLK_0" pad="J18"/>
<connect gate="G$1" pin="LCLK_1" pad="N18"/>
<connect gate="G$1" pin="LDAT0_0" pad="E18"/>
<connect gate="G$1" pin="LDAT0_1" pad="F17"/>
<connect gate="G$1" pin="LDAT0_2" pad="F18"/>
<connect gate="G$1" pin="LDAT0_3" pad="G17"/>
<connect gate="G$1" pin="LDAT0_4" pad="G18"/>
<connect gate="G$1" pin="LDAT0_5" pad="H16"/>
<connect gate="G$1" pin="LDAT0_6" pad="H17"/>
<connect gate="G$1" pin="LDAT0_7" pad="J16"/>
<connect gate="G$1" pin="LDAT1_0" pad="K18"/>
<connect gate="G$1" pin="LDAT1_1" pad="L16"/>
<connect gate="G$1" pin="LDAT1_2" pad="L17"/>
<connect gate="G$1" pin="LDAT1_3" pad="L18"/>
<connect gate="G$1" pin="LDAT1_4" pad="M16"/>
<connect gate="G$1" pin="LDAT1_5" pad="M17"/>
<connect gate="G$1" pin="LDAT1_6" pad="N16"/>
<connect gate="G$1" pin="LDAT1_7" pad="P16"/>
<connect gate="G$1" pin="MLBCLK" pad="K3"/>
<connect gate="G$1" pin="MLBDAT" pad="K4"/>
<connect gate="G$1" pin="MLBDO" pad="L4"/>
<connect gate="G$1" pin="MLBSIG" pad="L2"/>
<connect gate="G$1" pin="MLBSO" pad="L3"/>
<connect gate="G$1" pin="RESET_B" pad="M1"/>
<connect gate="G$1" pin="TCK" pad="K15"/>
<connect gate="G$1" pin="TDI" pad="L15"/>
<connect gate="G$1" pin="TDO" pad="M15"/>
<connect gate="G$1" pin="THD_M" pad="N12"/>
<connect gate="G$1" pin="THD_P" pad="N11"/>
<connect gate="G$1" pin="TMS" pad="K16"/>
<connect gate="G$1" pin="TRST_B" pad="N15"/>
<connect gate="G$1" pin="VDD_A" pad="H1"/>
<connect gate="G$1" pin="VDD_DDR2@0" pad="C5"/>
<connect gate="G$1" pin="VDD_DDR2@1" pad="C12"/>
<connect gate="G$1" pin="VDD_DDR2@10" pad="E11"/>
<connect gate="G$1" pin="VDD_DDR2@11" pad="E17"/>
<connect gate="G$1" pin="VDD_DDR2@12" pad="F3"/>
<connect gate="G$1" pin="VDD_DDR2@13" pad="F5"/>
<connect gate="G$1" pin="VDD_DDR2@14" pad="F15"/>
<connect gate="G$1" pin="VDD_DDR2@15" pad="G14"/>
<connect gate="G$1" pin="VDD_DDR2@16" pad="G16"/>
<connect gate="G$1" pin="VDD_DDR2@2" pad="D3"/>
<connect gate="G$1" pin="VDD_DDR2@3" pad="D6"/>
<connect gate="G$1" pin="VDD_DDR2@4" pad="D8"/>
<connect gate="G$1" pin="VDD_DDR2@5" pad="D18"/>
<connect gate="G$1" pin="VDD_DDR2@6" pad="E2"/>
<connect gate="G$1" pin="VDD_DDR2@7" pad="E4"/>
<connect gate="G$1" pin="VDD_DDR2@8" pad="E7"/>
<connect gate="G$1" pin="VDD_DDR2@9" pad="E10"/>
<connect gate="G$1" pin="VDD_EXT@0" pad="H15"/>
<connect gate="G$1" pin="VDD_EXT@1" pad="H18"/>
<connect gate="G$1" pin="VDD_EXT@10" pad="P8"/>
<connect gate="G$1" pin="VDD_EXT@11" pad="P10"/>
<connect gate="G$1" pin="VDD_EXT@12" pad="P12"/>
<connect gate="G$1" pin="VDD_EXT@13" pad="P14"/>
<connect gate="G$1" pin="VDD_EXT@14" pad="P15"/>
<connect gate="G$1" pin="VDD_EXT@15" pad="T8"/>
<connect gate="G$1" pin="VDD_EXT@16" pad="T9"/>
<connect gate="G$1" pin="VDD_EXT@17" pad="U8"/>
<connect gate="G$1" pin="VDD_EXT@18" pad="U9"/>
<connect gate="G$1" pin="VDD_EXT@19" pad="V8"/>
<connect gate="G$1" pin="VDD_EXT@2" pad="J5"/>
<connect gate="G$1" pin="VDD_EXT@20" pad="V9"/>
<connect gate="G$1" pin="VDD_EXT@3" pad="J15"/>
<connect gate="G$1" pin="VDD_EXT@4" pad="K14"/>
<connect gate="G$1" pin="VDD_EXT@5" pad="L5"/>
<connect gate="G$1" pin="VDD_EXT@6" pad="M14"/>
<connect gate="G$1" pin="VDD_EXT@7" pad="M18"/>
<connect gate="G$1" pin="VDD_EXT@8" pad="N5"/>
<connect gate="G$1" pin="VDD_EXT@9" pad="P6"/>
<connect gate="G$1" pin="VDD_INT@0" pad="D12"/>
<connect gate="G$1" pin="VDD_INT@1" pad="E6"/>
<connect gate="G$1" pin="VDD_INT@10" pad="F10"/>
<connect gate="G$1" pin="VDD_INT@11" pad="F11"/>
<connect gate="G$1" pin="VDD_INT@12" pad="F12"/>
<connect gate="G$1" pin="VDD_INT@13" pad="F13"/>
<connect gate="G$1" pin="VDD_INT@14" pad="G6"/>
<connect gate="G$1" pin="VDD_INT@15" pad="G13"/>
<connect gate="G$1" pin="VDD_INT@16" pad="H5"/>
<connect gate="G$1" pin="VDD_INT@17" pad="H6"/>
<connect gate="G$1" pin="VDD_INT@18" pad="H13"/>
<connect gate="G$1" pin="VDD_INT@19" pad="H14"/>
<connect gate="G$1" pin="VDD_INT@2" pad="E8"/>
<connect gate="G$1" pin="VDD_INT@20" pad="J6"/>
<connect gate="G$1" pin="VDD_INT@21" pad="J13"/>
<connect gate="G$1" pin="VDD_INT@22" pad="K6"/>
<connect gate="G$1" pin="VDD_INT@23" pad="K13"/>
<connect gate="G$1" pin="VDD_INT@24" pad="L6"/>
<connect gate="G$1" pin="VDD_INT@25" pad="L13"/>
<connect gate="G$1" pin="VDD_INT@26" pad="M6"/>
<connect gate="G$1" pin="VDD_INT@27" pad="M13"/>
<connect gate="G$1" pin="VDD_INT@28" pad="N6"/>
<connect gate="G$1" pin="VDD_INT@29" pad="N7"/>
<connect gate="G$1" pin="VDD_INT@3" pad="E9"/>
<connect gate="G$1" pin="VDD_INT@30" pad="N8"/>
<connect gate="G$1" pin="VDD_INT@31" pad="N9"/>
<connect gate="G$1" pin="VDD_INT@32" pad="N13"/>
<connect gate="G$1" pin="VDD_INT@4" pad="E14"/>
<connect gate="G$1" pin="VDD_INT@5" pad="E15"/>
<connect gate="G$1" pin="VDD_INT@6" pad="F6"/>
<connect gate="G$1" pin="VDD_INT@7" pad="F7"/>
<connect gate="G$1" pin="VDD_INT@8" pad="F8"/>
<connect gate="G$1" pin="VDD_INT@9" pad="F9"/>
<connect gate="G$1" pin="VDD_THD" pad="N10"/>
<connect gate="G$1" pin="VREF0" pad="D4"/>
<connect gate="G$1" pin="VREF1" pad="D11"/>
<connect gate="G$1" pin="XTAL" pad="K1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADSP_21467" prefix="IC">
<description>&lt;b&gt;SHARC Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: ADSP_21467_324_CSPBGA_bsdl.txt&lt;br&gt;
http://www.analog.com/static/imported-files/data_sheets/ADSP_21462W_21465W_21467_21469_21469W.pdf</description>
<gates>
<gate name="G$1" symbol="ADSP_21467"/>
</gates>
<devices>
<device name="" package="BGA_324_CSP">
<connects>
<connect gate="G$1" pin="AGND" pad="H2"/>
<connect gate="G$1" pin="AMI_ACK" pad="R10"/>
<connect gate="G$1" pin="AMI_ADDR0" pad="V16"/>
<connect gate="G$1" pin="AMI_ADDR01" pad="U16"/>
<connect gate="G$1" pin="AMI_ADDR02" pad="T16"/>
<connect gate="G$1" pin="AMI_ADDR03" pad="R16"/>
<connect gate="G$1" pin="AMI_ADDR04" pad="V15"/>
<connect gate="G$1" pin="AMI_ADDR05" pad="U15"/>
<connect gate="G$1" pin="AMI_ADDR06" pad="T15"/>
<connect gate="G$1" pin="AMI_ADDR07" pad="R15"/>
<connect gate="G$1" pin="AMI_ADDR08" pad="V14"/>
<connect gate="G$1" pin="AMI_ADDR09" pad="U14"/>
<connect gate="G$1" pin="AMI_ADDR10" pad="T14"/>
<connect gate="G$1" pin="AMI_ADDR11" pad="R14"/>
<connect gate="G$1" pin="AMI_ADDR12" pad="V13"/>
<connect gate="G$1" pin="AMI_ADDR13" pad="U13"/>
<connect gate="G$1" pin="AMI_ADDR14" pad="T13"/>
<connect gate="G$1" pin="AMI_ADDR15" pad="R13"/>
<connect gate="G$1" pin="AMI_ADDR16" pad="V12"/>
<connect gate="G$1" pin="AMI_ADDR17" pad="U12"/>
<connect gate="G$1" pin="AMI_ADDR18" pad="T12"/>
<connect gate="G$1" pin="AMI_ADDR19" pad="R12"/>
<connect gate="G$1" pin="AMI_ADDR20" pad="V11"/>
<connect gate="G$1" pin="AMI_ADDR21" pad="U11"/>
<connect gate="G$1" pin="AMI_ADDR22" pad="T11"/>
<connect gate="G$1" pin="AMI_ADDR23" pad="R11"/>
<connect gate="G$1" pin="AMI_DATA0" pad="U18"/>
<connect gate="G$1" pin="AMI_DATA1" pad="T18"/>
<connect gate="G$1" pin="AMI_DATA2" pad="R18"/>
<connect gate="G$1" pin="AMI_DATA3" pad="P18"/>
<connect gate="G$1" pin="AMI_DATA4" pad="V17"/>
<connect gate="G$1" pin="AMI_DATA5" pad="U17"/>
<connect gate="G$1" pin="AMI_DATA6" pad="T17"/>
<connect gate="G$1" pin="AMI_DATA7" pad="R17"/>
<connect gate="G$1" pin="AMI_MS0_B" pad="T10"/>
<connect gate="G$1" pin="AMI_MS1_B" pad="U10"/>
<connect gate="G$1" pin="AMI_RD_B" pad="J4"/>
<connect gate="G$1" pin="AMI_WR_B" pad="V10"/>
<connect gate="G$1" pin="BOOT_CFG0" pad="J2"/>
<connect gate="G$1" pin="BOOT_CFG1" pad="J3"/>
<connect gate="G$1" pin="BOOT_CFG2" pad="H3"/>
<connect gate="G$1" pin="CLKIN" pad="L1"/>
<connect gate="G$1" pin="CLKOUT" pad="M2"/>
<connect gate="G$1" pin="CLK_CFG0" pad="G1"/>
<connect gate="G$1" pin="CLK_CFG1" pad="G2"/>
<connect gate="G$1" pin="DAI_P01" pad="R6"/>
<connect gate="G$1" pin="DAI_P02" pad="V5"/>
<connect gate="G$1" pin="DAI_P03" pad="R7"/>
<connect gate="G$1" pin="DAI_P04" pad="R3"/>
<connect gate="G$1" pin="DAI_P05" pad="U5"/>
<connect gate="G$1" pin="DAI_P06" pad="T5"/>
<connect gate="G$1" pin="DAI_P07" pad="V6"/>
<connect gate="G$1" pin="DAI_P08" pad="V2"/>
<connect gate="G$1" pin="DAI_P09" pad="R5"/>
<connect gate="G$1" pin="DAI_P10" pad="V4"/>
<connect gate="G$1" pin="DAI_P11" pad="U4"/>
<connect gate="G$1" pin="DAI_P12" pad="T4"/>
<connect gate="G$1" pin="DAI_P13" pad="U6"/>
<connect gate="G$1" pin="DAI_P14" pad="U2"/>
<connect gate="G$1" pin="DAI_P15" pad="R4"/>
<connect gate="G$1" pin="DAI_P16" pad="V3"/>
<connect gate="G$1" pin="DAI_P17" pad="U3"/>
<connect gate="G$1" pin="DAI_P18" pad="T3"/>
<connect gate="G$1" pin="DAI_P19" pad="T6"/>
<connect gate="G$1" pin="DAI_P20" pad="T2"/>
<connect gate="G$1" pin="DDR2_ADDR0" pad="D13"/>
<connect gate="G$1" pin="DDR2_ADDR01" pad="C13"/>
<connect gate="G$1" pin="DDR2_ADDR02" pad="D14"/>
<connect gate="G$1" pin="DDR2_ADDR03" pad="C14"/>
<connect gate="G$1" pin="DDR2_ADDR04" pad="B14"/>
<connect gate="G$1" pin="DDR2_ADDR05" pad="A14"/>
<connect gate="G$1" pin="DDR2_ADDR06" pad="D15"/>
<connect gate="G$1" pin="DDR2_ADDR07" pad="C15"/>
<connect gate="G$1" pin="DDR2_ADDR08" pad="B15"/>
<connect gate="G$1" pin="DDR2_ADDR09" pad="A15"/>
<connect gate="G$1" pin="DDR2_ADDR10" pad="D16"/>
<connect gate="G$1" pin="DDR2_ADDR11" pad="C16"/>
<connect gate="G$1" pin="DDR2_ADDR12" pad="B16"/>
<connect gate="G$1" pin="DDR2_ADDR13" pad="A16"/>
<connect gate="G$1" pin="DDR2_ADDR14" pad="B17"/>
<connect gate="G$1" pin="DDR2_ADDR15" pad="A17"/>
<connect gate="G$1" pin="DDR2_BA0" pad="C18"/>
<connect gate="G$1" pin="DDR2_BA1" pad="C17"/>
<connect gate="G$1" pin="DDR2_BA2" pad="B18"/>
<connect gate="G$1" pin="DDR2_CAS_B" pad="C7"/>
<connect gate="G$1" pin="DDR2_CKE" pad="E1"/>
<connect gate="G$1" pin="DDR2_CLK0" pad="B7"/>
<connect gate="G$1" pin="DDR2_CLK0_B" pad="A7"/>
<connect gate="G$1" pin="DDR2_CLK1" pad="B13"/>
<connect gate="G$1" pin="DDR2_CLK1_B" pad="A13"/>
<connect gate="G$1" pin="DDR2_CS0_B" pad="C1"/>
<connect gate="G$1" pin="DDR2_CS1_B" pad="D1"/>
<connect gate="G$1" pin="DDR2_CS2_B" pad="C2"/>
<connect gate="G$1" pin="DDR2_CS3_B" pad="D2"/>
<connect gate="G$1" pin="DDR2_DATA0" pad="B2"/>
<connect gate="G$1" pin="DDR2_DATA01" pad="A2"/>
<connect gate="G$1" pin="DDR2_DATA02" pad="B3"/>
<connect gate="G$1" pin="DDR2_DATA03" pad="A3"/>
<connect gate="G$1" pin="DDR2_DATA04" pad="B5"/>
<connect gate="G$1" pin="DDR2_DATA05" pad="A5"/>
<connect gate="G$1" pin="DDR2_DATA06" pad="B6"/>
<connect gate="G$1" pin="DDR2_DATA07" pad="A6"/>
<connect gate="G$1" pin="DDR2_DATA08" pad="B8"/>
<connect gate="G$1" pin="DDR2_DATA09" pad="A8"/>
<connect gate="G$1" pin="DDR2_DATA10" pad="B9"/>
<connect gate="G$1" pin="DDR2_DATA11" pad="A9"/>
<connect gate="G$1" pin="DDR2_DATA12" pad="A11"/>
<connect gate="G$1" pin="DDR2_DATA13" pad="B11"/>
<connect gate="G$1" pin="DDR2_DATA14" pad="A12"/>
<connect gate="G$1" pin="DDR2_DATA15" pad="B12"/>
<connect gate="G$1" pin="DDR2_DM0" pad="C3"/>
<connect gate="G$1" pin="DDR2_DM1" pad="C11"/>
<connect gate="G$1" pin="DDR2_DQS0" pad="A4"/>
<connect gate="G$1" pin="DDR2_DQS0_B" pad="B4"/>
<connect gate="G$1" pin="DDR2_DQS1" pad="A10"/>
<connect gate="G$1" pin="DDR2_DQS1_B" pad="B10"/>
<connect gate="G$1" pin="DDR2_ODT" pad="B1"/>
<connect gate="G$1" pin="DDR2_RAS_B" pad="C9"/>
<connect gate="G$1" pin="DDR2_WE_B" pad="C10"/>
<connect gate="G$1" pin="DPI_P01" pad="R2"/>
<connect gate="G$1" pin="DPI_P02" pad="U1"/>
<connect gate="G$1" pin="DPI_P03" pad="T1"/>
<connect gate="G$1" pin="DPI_P04" pad="R1"/>
<connect gate="G$1" pin="DPI_P05" pad="P1"/>
<connect gate="G$1" pin="DPI_P06" pad="P2"/>
<connect gate="G$1" pin="DPI_P07" pad="P3"/>
<connect gate="G$1" pin="DPI_P08" pad="P4"/>
<connect gate="G$1" pin="DPI_P09" pad="N1"/>
<connect gate="G$1" pin="DPI_P10" pad="N2"/>
<connect gate="G$1" pin="DPI_P11" pad="N3"/>
<connect gate="G$1" pin="DPI_P12" pad="N4"/>
<connect gate="G$1" pin="DPI_P13" pad="M3"/>
<connect gate="G$1" pin="DPI_P14" pad="M4"/>
<connect gate="G$1" pin="EMU_B" pad="K2"/>
<connect gate="G$1" pin="FLAG0" pad="R8"/>
<connect gate="G$1" pin="FLAG1" pad="V7"/>
<connect gate="G$1" pin="FLAG2" pad="U7"/>
<connect gate="G$1" pin="FLAG3" pad="T7"/>
<connect gate="G$1" pin="GND@0" pad="A1"/>
<connect gate="G$1" pin="GND@1" pad="A18"/>
<connect gate="G$1" pin="GND@10" pad="E3"/>
<connect gate="G$1" pin="GND@11" pad="E5"/>
<connect gate="G$1" pin="GND@12" pad="E12"/>
<connect gate="G$1" pin="GND@13" pad="E13"/>
<connect gate="G$1" pin="GND@14" pad="E16"/>
<connect gate="G$1" pin="GND@15" pad="F1"/>
<connect gate="G$1" pin="GND@16" pad="F2"/>
<connect gate="G$1" pin="GND@17" pad="F4"/>
<connect gate="G$1" pin="GND@18" pad="F14"/>
<connect gate="G$1" pin="GND@19" pad="F16"/>
<connect gate="G$1" pin="GND@2" pad="C4"/>
<connect gate="G$1" pin="GND@20" pad="G3"/>
<connect gate="G$1" pin="GND@21" pad="G4"/>
<connect gate="G$1" pin="GND@22" pad="G5"/>
<connect gate="G$1" pin="GND@23" pad="G7"/>
<connect gate="G$1" pin="GND@24" pad="G8"/>
<connect gate="G$1" pin="GND@25" pad="G9"/>
<connect gate="G$1" pin="GND@26" pad="G10"/>
<connect gate="G$1" pin="GND@27" pad="G11"/>
<connect gate="G$1" pin="GND@28" pad="G12"/>
<connect gate="G$1" pin="GND@29" pad="G15"/>
<connect gate="G$1" pin="GND@3" pad="C6"/>
<connect gate="G$1" pin="GND@30" pad="H4"/>
<connect gate="G$1" pin="GND@31" pad="H7"/>
<connect gate="G$1" pin="GND@32" pad="H8"/>
<connect gate="G$1" pin="GND@33" pad="H9"/>
<connect gate="G$1" pin="GND@34" pad="H10"/>
<connect gate="G$1" pin="GND@35" pad="H11"/>
<connect gate="G$1" pin="GND@36" pad="H12"/>
<connect gate="G$1" pin="GND@37" pad="J1"/>
<connect gate="G$1" pin="GND@38" pad="J7"/>
<connect gate="G$1" pin="GND@39" pad="J8"/>
<connect gate="G$1" pin="GND@4" pad="C8"/>
<connect gate="G$1" pin="GND@40" pad="J9"/>
<connect gate="G$1" pin="GND@41" pad="J10"/>
<connect gate="G$1" pin="GND@42" pad="J11"/>
<connect gate="G$1" pin="GND@43" pad="J12"/>
<connect gate="G$1" pin="GND@44" pad="J14"/>
<connect gate="G$1" pin="GND@45" pad="J17"/>
<connect gate="G$1" pin="GND@46" pad="K5"/>
<connect gate="G$1" pin="GND@47" pad="K7"/>
<connect gate="G$1" pin="GND@48" pad="K8"/>
<connect gate="G$1" pin="GND@49" pad="K9"/>
<connect gate="G$1" pin="GND@5" pad="D5"/>
<connect gate="G$1" pin="GND@50" pad="K10"/>
<connect gate="G$1" pin="GND@51" pad="K11"/>
<connect gate="G$1" pin="GND@52" pad="K12"/>
<connect gate="G$1" pin="GND@53" pad="L7"/>
<connect gate="G$1" pin="GND@54" pad="L8"/>
<connect gate="G$1" pin="GND@55" pad="L9"/>
<connect gate="G$1" pin="GND@56" pad="L10"/>
<connect gate="G$1" pin="GND@57" pad="L11"/>
<connect gate="G$1" pin="GND@58" pad="L12"/>
<connect gate="G$1" pin="GND@59" pad="L14"/>
<connect gate="G$1" pin="GND@6" pad="D7"/>
<connect gate="G$1" pin="GND@60" pad="M5"/>
<connect gate="G$1" pin="GND@61" pad="M7"/>
<connect gate="G$1" pin="GND@62" pad="M8"/>
<connect gate="G$1" pin="GND@63" pad="M9"/>
<connect gate="G$1" pin="GND@64" pad="M10"/>
<connect gate="G$1" pin="GND@65" pad="M11"/>
<connect gate="G$1" pin="GND@66" pad="M12"/>
<connect gate="G$1" pin="GND@67" pad="N14"/>
<connect gate="G$1" pin="GND@68" pad="N17"/>
<connect gate="G$1" pin="GND@69" pad="P5"/>
<connect gate="G$1" pin="GND@7" pad="D9"/>
<connect gate="G$1" pin="GND@70" pad="P7"/>
<connect gate="G$1" pin="GND@71" pad="P9"/>
<connect gate="G$1" pin="GND@72" pad="P11"/>
<connect gate="G$1" pin="GND@73" pad="P13"/>
<connect gate="G$1" pin="GND@74" pad="R9"/>
<connect gate="G$1" pin="GND@75" pad="V1"/>
<connect gate="G$1" pin="GND@76" pad="V18"/>
<connect gate="G$1" pin="GND@8" pad="D10"/>
<connect gate="G$1" pin="GND@9" pad="D17"/>
<connect gate="G$1" pin="LACK_0" pad="K17"/>
<connect gate="G$1" pin="LACK_1" pad="P17"/>
<connect gate="G$1" pin="LCLK_0" pad="J18"/>
<connect gate="G$1" pin="LCLK_1" pad="N18"/>
<connect gate="G$1" pin="LDAT0_0" pad="E18"/>
<connect gate="G$1" pin="LDAT0_1" pad="F17"/>
<connect gate="G$1" pin="LDAT0_2" pad="F18"/>
<connect gate="G$1" pin="LDAT0_3" pad="G17"/>
<connect gate="G$1" pin="LDAT0_4" pad="G18"/>
<connect gate="G$1" pin="LDAT0_5" pad="H16"/>
<connect gate="G$1" pin="LDAT0_6" pad="H17"/>
<connect gate="G$1" pin="LDAT0_7" pad="J16"/>
<connect gate="G$1" pin="LDAT1_0" pad="K18"/>
<connect gate="G$1" pin="LDAT1_1" pad="L16"/>
<connect gate="G$1" pin="LDAT1_2" pad="L17"/>
<connect gate="G$1" pin="LDAT1_3" pad="L18"/>
<connect gate="G$1" pin="LDAT1_4" pad="M16"/>
<connect gate="G$1" pin="LDAT1_5" pad="M17"/>
<connect gate="G$1" pin="LDAT1_6" pad="N16"/>
<connect gate="G$1" pin="LDAT1_7" pad="P16"/>
<connect gate="G$1" pin="NC0" pad="K3"/>
<connect gate="G$1" pin="NC1" pad="K4"/>
<connect gate="G$1" pin="NC2" pad="L2"/>
<connect gate="G$1" pin="NC3" pad="L3"/>
<connect gate="G$1" pin="NC4" pad="L4"/>
<connect gate="G$1" pin="RESET_B" pad="M1"/>
<connect gate="G$1" pin="TCK" pad="K15"/>
<connect gate="G$1" pin="TDI" pad="L15"/>
<connect gate="G$1" pin="TDO" pad="M15"/>
<connect gate="G$1" pin="THD_M" pad="N12"/>
<connect gate="G$1" pin="THD_P" pad="N11"/>
<connect gate="G$1" pin="TMS" pad="K16"/>
<connect gate="G$1" pin="TRST_B" pad="N15"/>
<connect gate="G$1" pin="VDD_A" pad="H1"/>
<connect gate="G$1" pin="VDD_DDR2@0" pad="C5"/>
<connect gate="G$1" pin="VDD_DDR2@1" pad="C12"/>
<connect gate="G$1" pin="VDD_DDR2@10" pad="E11"/>
<connect gate="G$1" pin="VDD_DDR2@11" pad="E17"/>
<connect gate="G$1" pin="VDD_DDR2@12" pad="F3"/>
<connect gate="G$1" pin="VDD_DDR2@13" pad="F5"/>
<connect gate="G$1" pin="VDD_DDR2@14" pad="F15"/>
<connect gate="G$1" pin="VDD_DDR2@15" pad="G14"/>
<connect gate="G$1" pin="VDD_DDR2@16" pad="G16"/>
<connect gate="G$1" pin="VDD_DDR2@2" pad="D3"/>
<connect gate="G$1" pin="VDD_DDR2@3" pad="D6"/>
<connect gate="G$1" pin="VDD_DDR2@4" pad="D8"/>
<connect gate="G$1" pin="VDD_DDR2@5" pad="D18"/>
<connect gate="G$1" pin="VDD_DDR2@6" pad="E2"/>
<connect gate="G$1" pin="VDD_DDR2@7" pad="E4"/>
<connect gate="G$1" pin="VDD_DDR2@8" pad="E7"/>
<connect gate="G$1" pin="VDD_DDR2@9" pad="E10"/>
<connect gate="G$1" pin="VDD_EXT@0" pad="H15"/>
<connect gate="G$1" pin="VDD_EXT@1" pad="H18"/>
<connect gate="G$1" pin="VDD_EXT@10" pad="P8"/>
<connect gate="G$1" pin="VDD_EXT@11" pad="P10"/>
<connect gate="G$1" pin="VDD_EXT@12" pad="P12"/>
<connect gate="G$1" pin="VDD_EXT@13" pad="P14"/>
<connect gate="G$1" pin="VDD_EXT@14" pad="P15"/>
<connect gate="G$1" pin="VDD_EXT@15" pad="T8"/>
<connect gate="G$1" pin="VDD_EXT@16" pad="T9"/>
<connect gate="G$1" pin="VDD_EXT@17" pad="U8"/>
<connect gate="G$1" pin="VDD_EXT@18" pad="U9"/>
<connect gate="G$1" pin="VDD_EXT@19" pad="V8"/>
<connect gate="G$1" pin="VDD_EXT@2" pad="J5"/>
<connect gate="G$1" pin="VDD_EXT@20" pad="V9"/>
<connect gate="G$1" pin="VDD_EXT@3" pad="J15"/>
<connect gate="G$1" pin="VDD_EXT@4" pad="K14"/>
<connect gate="G$1" pin="VDD_EXT@5" pad="L5"/>
<connect gate="G$1" pin="VDD_EXT@6" pad="M14"/>
<connect gate="G$1" pin="VDD_EXT@7" pad="M18"/>
<connect gate="G$1" pin="VDD_EXT@8" pad="N5"/>
<connect gate="G$1" pin="VDD_EXT@9" pad="P6"/>
<connect gate="G$1" pin="VDD_INT@0" pad="D12"/>
<connect gate="G$1" pin="VDD_INT@1" pad="E6"/>
<connect gate="G$1" pin="VDD_INT@10" pad="F10"/>
<connect gate="G$1" pin="VDD_INT@11" pad="F11"/>
<connect gate="G$1" pin="VDD_INT@12" pad="F12"/>
<connect gate="G$1" pin="VDD_INT@13" pad="F13"/>
<connect gate="G$1" pin="VDD_INT@14" pad="G6"/>
<connect gate="G$1" pin="VDD_INT@15" pad="G13"/>
<connect gate="G$1" pin="VDD_INT@16" pad="H5"/>
<connect gate="G$1" pin="VDD_INT@17" pad="H6"/>
<connect gate="G$1" pin="VDD_INT@18" pad="H13"/>
<connect gate="G$1" pin="VDD_INT@19" pad="H14"/>
<connect gate="G$1" pin="VDD_INT@2" pad="E8"/>
<connect gate="G$1" pin="VDD_INT@20" pad="J6"/>
<connect gate="G$1" pin="VDD_INT@21" pad="J13"/>
<connect gate="G$1" pin="VDD_INT@22" pad="K6"/>
<connect gate="G$1" pin="VDD_INT@23" pad="K13"/>
<connect gate="G$1" pin="VDD_INT@24" pad="L6"/>
<connect gate="G$1" pin="VDD_INT@25" pad="L13"/>
<connect gate="G$1" pin="VDD_INT@26" pad="M6"/>
<connect gate="G$1" pin="VDD_INT@27" pad="M13"/>
<connect gate="G$1" pin="VDD_INT@28" pad="N6"/>
<connect gate="G$1" pin="VDD_INT@29" pad="N7"/>
<connect gate="G$1" pin="VDD_INT@3" pad="E9"/>
<connect gate="G$1" pin="VDD_INT@30" pad="N8"/>
<connect gate="G$1" pin="VDD_INT@31" pad="N9"/>
<connect gate="G$1" pin="VDD_INT@32" pad="N13"/>
<connect gate="G$1" pin="VDD_INT@4" pad="E14"/>
<connect gate="G$1" pin="VDD_INT@5" pad="E15"/>
<connect gate="G$1" pin="VDD_INT@6" pad="F6"/>
<connect gate="G$1" pin="VDD_INT@7" pad="F7"/>
<connect gate="G$1" pin="VDD_INT@8" pad="F8"/>
<connect gate="G$1" pin="VDD_INT@9" pad="F9"/>
<connect gate="G$1" pin="VDD_THD" pad="N10"/>
<connect gate="G$1" pin="VREF0" pad="D4"/>
<connect gate="G$1" pin="VREF1" pad="D11"/>
<connect gate="G$1" pin="XTAL" pad="K1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADV7184" prefix="IC">
<description>&lt;b&gt;Multiformat SDTV Video Decoder with Fast Switch Overlay Support&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADV7184.pdf</description>
<gates>
<gate name="G$1" symbol="ADV7184"/>
</gates>
<devices>
<device name="" package="LQFP80">
<connects>
<connect gate="G$1" pin="AGND" pad="39"/>
<connect gate="G$1" pin="AGND@1" pad="47"/>
<connect gate="G$1" pin="AGND@2" pad="53"/>
<connect gate="G$1" pin="AGND@3" pad="56"/>
<connect gate="G$1" pin="AIN1" pad="42"/>
<connect gate="G$1" pin="AIN10" pad="57"/>
<connect gate="G$1" pin="AIN11" pad="59"/>
<connect gate="G$1" pin="AIN12" pad="61"/>
<connect gate="G$1" pin="AIN2" pad="44"/>
<connect gate="G$1" pin="AIN3" pad="46"/>
<connect gate="G$1" pin="AIN4" pad="58"/>
<connect gate="G$1" pin="AIN5" pad="60"/>
<connect gate="G$1" pin="AIN6" pad="62"/>
<connect gate="G$1" pin="AIN7" pad="41"/>
<connect gate="G$1" pin="AIN8" pad="43"/>
<connect gate="G$1" pin="AIN9" pad="45"/>
<connect gate="G$1" pin="ALSB" pad="66"/>
<connect gate="G$1" pin="AVDD" pad="50"/>
<connect gate="G$1" pin="CAPC1" pad="54"/>
<connect gate="G$1" pin="CAPC2" pad="55"/>
<connect gate="G$1" pin="CAPY1" pad="48"/>
<connect gate="G$1" pin="CAPY2" pad="49"/>
<connect gate="G$1" pin="CML" pad="52"/>
<connect gate="G$1" pin="DGND" pad="3"/>
<connect gate="G$1" pin="DGND@1" pad="9"/>
<connect gate="G$1" pin="DGND@2" pad="14"/>
<connect gate="G$1" pin="DGND@3" pad="31"/>
<connect gate="G$1" pin="DGND@4" pad="71"/>
<connect gate="G$1" pin="DVDD" pad="10"/>
<connect gate="G$1" pin="DVDD@1" pad="30"/>
<connect gate="G$1" pin="DVDD@2" pad="72"/>
<connect gate="G$1" pin="DVDDIO" pad="4"/>
<connect gate="G$1" pin="DVDDIO@1" pad="15"/>
<connect gate="G$1" pin="ELPF" pad="37"/>
<connect gate="G$1" pin="FB" pad="40"/>
<connect gate="G$1" pin="FIELD" pad="80"/>
<connect gate="G$1" pin="HS" pad="2"/>
<connect gate="G$1" pin="INT" pad="11"/>
<connect gate="G$1" pin="LLC1" pad="27"/>
<connect gate="G$1" pin="LLC2" pad="26"/>
<connect gate="G$1" pin="OE" pad="79"/>
<connect gate="G$1" pin="P0" pad="33"/>
<connect gate="G$1" pin="P1" pad="32"/>
<connect gate="G$1" pin="P10" pad="6"/>
<connect gate="G$1" pin="P11" pad="5"/>
<connect gate="G$1" pin="P12" pad="76"/>
<connect gate="G$1" pin="P13" pad="75"/>
<connect gate="G$1" pin="P14" pad="74"/>
<connect gate="G$1" pin="P15" pad="73"/>
<connect gate="G$1" pin="P2" pad="24"/>
<connect gate="G$1" pin="P3" pad="23"/>
<connect gate="G$1" pin="P4" pad="22"/>
<connect gate="G$1" pin="P5" pad="21"/>
<connect gate="G$1" pin="P6" pad="20"/>
<connect gate="G$1" pin="P7" pad="19"/>
<connect gate="G$1" pin="P8" pad="8"/>
<connect gate="G$1" pin="P9" pad="7"/>
<connect gate="G$1" pin="PVDD" pad="38"/>
<connect gate="G$1" pin="PWRDN" pad="36"/>
<connect gate="G$1" pin="REFOUT" pad="51"/>
<connect gate="G$1" pin="RESET" pad="64"/>
<connect gate="G$1" pin="SCLK" pad="68"/>
<connect gate="G$1" pin="SDA" pad="67"/>
<connect gate="G$1" pin="SFL" pad="12"/>
<connect gate="G$1" pin="SOY" pad="63"/>
<connect gate="G$1" pin="TEST0" pad="70"/>
<connect gate="G$1" pin="TEST1" pad="78"/>
<connect gate="G$1" pin="TEST10" pad="34"/>
<connect gate="G$1" pin="TEST11" pad="18"/>
<connect gate="G$1" pin="TEST12" pad="17"/>
<connect gate="G$1" pin="TEST2" pad="13"/>
<connect gate="G$1" pin="TEST3" pad="25"/>
<connect gate="G$1" pin="TEST4" pad="69"/>
<connect gate="G$1" pin="TEST6" pad="77"/>
<connect gate="G$1" pin="TEST7" pad="65"/>
<connect gate="G$1" pin="TEST8" pad="16"/>
<connect gate="G$1" pin="TEST9" pad="35"/>
<connect gate="G$1" pin="VS" pad="1"/>
<connect gate="G$1" pin="XTAL" pad="29"/>
<connect gate="G$1" pin="XTAL1" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADV7184BSTZ"/>
<attribute name="OC_FARNELL" value="1117101"/>
<attribute name="OC_NEWARK" value="31M3981"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADV7194" prefix="IC">
<description>&lt;b&gt;Professional Extended-10 (TM) Video Encoder with 54 MHz Oversampling&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADV7194.pdf</description>
<gates>
<gate name="G$1" symbol="ADV7194"/>
</gates>
<devices>
<device name="" package="LQFP80">
<connects>
<connect gate="G$1" pin="AGND" pad="35"/>
<connect gate="G$1" pin="AGND@1" pad="49"/>
<connect gate="G$1" pin="AGND@2" pad="52"/>
<connect gate="G$1" pin="ALSB" pad="42"/>
<connect gate="G$1" pin="BLANK" pad="25"/>
<connect gate="G$1" pin="CB0" pad="26"/>
<connect gate="G$1" pin="CB1" pad="27"/>
<connect gate="G$1" pin="CB2" pad="28"/>
<connect gate="G$1" pin="CB3" pad="29"/>
<connect gate="G$1" pin="CB4" pad="30"/>
<connect gate="G$1" pin="CB5" pad="31"/>
<connect gate="G$1" pin="CB6" pad="75"/>
<connect gate="G$1" pin="CB7" pad="76"/>
<connect gate="G$1" pin="CB8" pad="77"/>
<connect gate="G$1" pin="CB9" pad="78"/>
<connect gate="G$1" pin="CLKIN" pad="36"/>
<connect gate="G$1" pin="CLKOUT" pad="37"/>
<connect gate="G$1" pin="COMP2" pad="45"/>
<connect gate="G$1" pin="COMP_1" pad="56"/>
<connect gate="G$1" pin="CR0" pad="63"/>
<connect gate="G$1" pin="CR1" pad="64"/>
<connect gate="G$1" pin="CR2" pad="65"/>
<connect gate="G$1" pin="CR3" pad="66"/>
<connect gate="G$1" pin="CR4" pad="67"/>
<connect gate="G$1" pin="CR5" pad="70"/>
<connect gate="G$1" pin="CR6" pad="71"/>
<connect gate="G$1" pin="CR7" pad="72"/>
<connect gate="G$1" pin="CR8" pad="73"/>
<connect gate="G$1" pin="CR9" pad="74"/>
<connect gate="G$1" pin="CSO_HSO" pad="61"/>
<connect gate="G$1" pin="DAC_A" pad="55"/>
<connect gate="G$1" pin="DAC_B" pad="54"/>
<connect gate="G$1" pin="DAC_C" pad="51"/>
<connect gate="G$1" pin="DAC_D" pad="50"/>
<connect gate="G$1" pin="DAC_E" pad="47"/>
<connect gate="G$1" pin="DAC_F" pad="46"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="DGND@1" pad="33"/>
<connect gate="G$1" pin="DGND@2" pad="43"/>
<connect gate="G$1" pin="DGND@3" pad="69"/>
<connect gate="G$1" pin="DGND@4" pad="80"/>
<connect gate="G$1" pin="HSYNC" pad="23"/>
<connect gate="G$1" pin="P0" pad="1"/>
<connect gate="G$1" pin="P1" pad="2"/>
<connect gate="G$1" pin="P2" pad="3"/>
<connect gate="G$1" pin="P3" pad="4"/>
<connect gate="G$1" pin="P4" pad="5"/>
<connect gate="G$1" pin="P5" pad="6"/>
<connect gate="G$1" pin="P6" pad="7"/>
<connect gate="G$1" pin="P7" pad="8"/>
<connect gate="G$1" pin="P8" pad="9"/>
<connect gate="G$1" pin="P9" pad="10"/>
<connect gate="G$1" pin="PAL_NTSC" pad="59"/>
<connect gate="G$1" pin="RESET" pad="60"/>
<connect gate="G$1" pin="RSET1" pad="58"/>
<connect gate="G$1" pin="RSET2" pad="44"/>
<connect gate="G$1" pin="SCL" pad="39"/>
<connect gate="G$1" pin="SCRESET/RTC/TR" pad="41"/>
<connect gate="G$1" pin="SDA" pad="40"/>
<connect gate="G$1" pin="TTXREQ" pad="32"/>
<connect gate="G$1" pin="VAA" pad="38"/>
<connect gate="G$1" pin="VAA@1" pad="48"/>
<connect gate="G$1" pin="VAA@2" pad="53"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VDD@1" pad="34"/>
<connect gate="G$1" pin="VDD@2" pad="68"/>
<connect gate="G$1" pin="VDD@3" pad="79"/>
<connect gate="G$1" pin="VREF" pad="57"/>
<connect gate="G$1" pin="VSO/TTX/CLAMP" pad="62"/>
<connect gate="G$1" pin="VSYNC" pad="24"/>
<connect gate="G$1" pin="Y0/P10" pad="11"/>
<connect gate="G$1" pin="Y1/P11" pad="12"/>
<connect gate="G$1" pin="Y2/P12" pad="13"/>
<connect gate="G$1" pin="Y3/P13" pad="14"/>
<connect gate="G$1" pin="Y4/P14" pad="15"/>
<connect gate="G$1" pin="Y5/P15" pad="16"/>
<connect gate="G$1" pin="Y6/P16" pad="17"/>
<connect gate="G$1" pin="Y7/P17" pad="18"/>
<connect gate="G$1" pin="Y8/P18" pad="19"/>
<connect gate="G$1" pin="Y9/P19" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADV7194KSTZ"/>
<attribute name="OC_FARNELL" value="1438743"/>
<attribute name="OC_NEWARK" value="39P9724"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUF04" prefix="IC">
<description>&lt;b&gt;Closed-Loop High Speed Buffer&lt;/b&gt;&lt;font color="red"&gt; OBSOLETE&lt;/font&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets_obsolete/820549BUF04.pdf</description>
<gates>
<gate name="G$1" symbol="BUF+-OFF"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SO8">
<connects>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="-VS" pad="4"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OFF@1" pad="1"/>
<connect gate="G$1" pin="OFF@2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAT04" prefix="IC">
<description>&lt;b&gt;Matched Monolithic Quad Transistor&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/MAT04.pdf</description>
<gates>
<gate name="A" symbol="NPN+DIODE"/>
<gate name="B" symbol="NPN+DIODE"/>
<gate name="C" symbol="NPN+DIODE"/>
<gate name="D" symbol="NPN+DIODE"/>
<gate name="S" symbol="SUB"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="B" pin="B" pad="6"/>
<connect gate="B" pin="C" pad="7"/>
<connect gate="B" pin="E" pad="5"/>
<connect gate="C" pin="B" pad="9"/>
<connect gate="C" pin="C" pad="8"/>
<connect gate="C" pin="E" pad="10"/>
<connect gate="D" pin="B" pad="13"/>
<connect gate="D" pin="C" pad="14"/>
<connect gate="D" pin="E" pad="12"/>
<connect gate="S" pin="SUB@1" pad="4"/>
<connect gate="S" pin="SUB@2" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1465698"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SO14">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="B" pin="B" pad="6"/>
<connect gate="B" pin="C" pad="7"/>
<connect gate="B" pin="E" pad="5"/>
<connect gate="C" pin="B" pad="9"/>
<connect gate="C" pin="C" pad="8"/>
<connect gate="C" pin="E" pad="10"/>
<connect gate="D" pin="B" pad="13"/>
<connect gate="D" pin="C" pad="14"/>
<connect gate="D" pin="E" pad="12"/>
<connect gate="S" pin="SUB@1" pad="4"/>
<connect gate="S" pin="SUB@2" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MAT04FS"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="66F5730"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8235" prefix="IC">
<description>&lt;b&gt;40 ?A Micropower Instrumentation Amplifier in WLCSP Package&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8235.pdf</description>
<gates>
<gate name="G$1" symbol="AD8235"/>
</gates>
<devices>
<device name="" package="BGA_CB11">
<connects>
<connect gate="G$1" pin="+VS" pad="A1"/>
<connect gate="G$1" pin="-VS" pad="D1"/>
<connect gate="G$1" pin="IN+" pad="D3"/>
<connect gate="G$1" pin="IN-" pad="A3"/>
<connect gate="G$1" pin="REF" pad="C1"/>
<connect gate="G$1" pin="RG@1" pad="C3"/>
<connect gate="G$1" pin="RG@2" pad="B3"/>
<connect gate="G$1" pin="SDN" pad="A2"/>
<connect gate="G$1" pin="VOUT" pad="B1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8235ACBZ-P7"/>
<attribute name="OC_FARNELL" value="1827361"/>
<attribute name="OC_NEWARK" value="35R0266"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8603" prefix="IC">
<description>&lt;b&gt;Precision Micropower, Low Noise CMOS, Rail-to-Rail Input/Output Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8603_8607_8609.pdf</description>
<gates>
<gate name="G$1" symbol="OP+-VS"/>
</gates>
<devices>
<device name="UJ" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+VS" pad="5"/>
<connect gate="G$1" pin="-VS" pad="2"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8603AUJZ-REEL7"/>
<attribute name="OC_FARNELL" value="1651290"/>
<attribute name="OC_NEWARK" value="59K6904"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8607" prefix="IC">
<description>&lt;b&gt;Precision Micropower, Low Noise CMOS, Rail-to-Rail Input/Output Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8603_8607_8609.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="RM" package="MSOP08">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8607ARMZ-REEL"/>
<attribute name="OC_FARNELL" value="1464990"/>
<attribute name="OC_NEWARK" value="59K6925"/>
</technology>
</technologies>
</device>
<device name="R" package="SO8">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8607ARMZ-R2"/>
<attribute name="OC_FARNELL" value="1651293"/>
<attribute name="OC_NEWARK" value="19M8927"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8609" prefix="IC">
<description>&lt;b&gt;Precision Micropower, Low Noise CMOS, Rail-to-Rail Input/Output Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD8603_8607_8609.pdf</description>
<gates>
<gate name="A" symbol="OP"/>
<gate name="B" symbol="OP"/>
<gate name="C" symbol="OP"/>
<gate name="D" symbol="OP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="RU" package="TSSOP14">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="IN+" pad="10"/>
<connect gate="C" pin="IN-" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="IN+" pad="12"/>
<connect gate="D" pin="IN-" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8609ARUZ"/>
<attribute name="OC_FARNELL" value="1464994"/>
<attribute name="OC_NEWARK" value="59K6934"/>
</technology>
</technologies>
</device>
<device name="R" package="SO14">
<connects>
<connect gate="A" pin="IN+" pad="3"/>
<connect gate="A" pin="IN-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="IN+" pad="5"/>
<connect gate="B" pin="IN-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="IN+" pad="10"/>
<connect gate="C" pin="IN-" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="IN+" pad="12"/>
<connect gate="D" pin="IN-" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8609ARZ"/>
<attribute name="OC_FARNELL" value="1581951"/>
<attribute name="OC_NEWARK" value="19M0976"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD5282" prefix="IC">
<description>&lt;b&gt;Dual +15 V/±5 V, 256-Position, I2C-Compatible Digital Potentiometer&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD5280_5282.pdf</description>
<gates>
<gate name="G$1" symbol="AD5282"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!SHDN" pad="6"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="16"/>
<connect gate="G$1" pin="AD0" pad="9"/>
<connect gate="G$1" pin="AD1" pad="10"/>
<connect gate="G$1" pin="B1" pad="4"/>
<connect gate="G$1" pin="B2" pad="14"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="O1" pad="1"/>
<connect gate="G$1" pin="SCL" pad="7"/>
<connect gate="G$1" pin="SDA" pad="8"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VL" pad="13"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="W1" pad="3"/>
<connect gate="G$1" pin="W2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD5282BRUZ50"/>
<attribute name="OC_FARNELL" value="1438442"/>
<attribute name="OC_NEWARK" value="59K3850"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD5280" prefix="IC">
<description>&lt;b&gt;Single +15 V/±5 V, 256-Position, I2C-Compatible Digital Potentiometer&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD5280_5282.pdf</description>
<gates>
<gate name="G$1" symbol="AD5280"/>
</gates>
<devices>
<device name="" package="TSSOP14">
<connects>
<connect gate="G$1" pin="!SHDN" pad="5"/>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="AD0" pad="8"/>
<connect gate="G$1" pin="AD1" pad="9"/>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="O1" pad="14"/>
<connect gate="G$1" pin="O2" pad="12"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="7"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VL" pad="13"/>
<connect gate="G$1" pin="VSS" pad="11"/>
<connect gate="G$1" pin="W" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD5280BRUZ20"/>
<attribute name="OC_FARNELL" value="1464325"/>
<attribute name="OC_NEWARK" value="59K3840"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9854" prefix="IC">
<description>&lt;b&gt;CMOS 300 MSPS Quadrature Complete DDS&lt;/bY&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/AD9854.pdf</description>
<gates>
<gate name="G$1" symbol="AD9854"/>
</gates>
<devices>
<device name="" package="LQFP80">
<connects>
<connect gate="G$1" pin="!IOUT1" pad="49"/>
<connect gate="G$1" pin="!IOUT2" pad="51"/>
<connect gate="G$1" pin="!RD!/!CS!" pad="22"/>
<connect gate="G$1" pin="!REFCLK" pad="68"/>
<connect gate="G$1" pin="!WR!/SCLK" pad="21"/>
<connect gate="G$1" pin="A0/SDIO" pad="19"/>
<connect gate="G$1" pin="A1/SDO" pad="18"/>
<connect gate="G$1" pin="A2/IO_RESET" pad="17"/>
<connect gate="G$1" pin="A3" pad="16"/>
<connect gate="G$1" pin="A4" pad="15"/>
<connect gate="G$1" pin="A5" pad="14"/>
<connect gate="G$1" pin="AGND@1" pad="33"/>
<connect gate="G$1" pin="AGND@10" pad="59"/>
<connect gate="G$1" pin="AGND@11" pad="62"/>
<connect gate="G$1" pin="AGND@12" pad="66"/>
<connect gate="G$1" pin="AGND@13" pad="67"/>
<connect gate="G$1" pin="AGND@2" pad="34"/>
<connect gate="G$1" pin="AGND@3" pad="39"/>
<connect gate="G$1" pin="AGND@4" pad="40"/>
<connect gate="G$1" pin="AGND@5" pad="41"/>
<connect gate="G$1" pin="AGND@6" pad="45"/>
<connect gate="G$1" pin="AGND@7" pad="46"/>
<connect gate="G$1" pin="AGND@8" pad="47"/>
<connect gate="G$1" pin="AGND@9" pad="53"/>
<connect gate="G$1" pin="AVDD@1" pad="31"/>
<connect gate="G$1" pin="AVDD@2" pad="32"/>
<connect gate="G$1" pin="AVDD@3" pad="37"/>
<connect gate="G$1" pin="AVDD@4" pad="38"/>
<connect gate="G$1" pin="AVDD@5" pad="44"/>
<connect gate="G$1" pin="AVDD@6" pad="50"/>
<connect gate="G$1" pin="AVDD@7" pad="54"/>
<connect gate="G$1" pin="AVDD@8" pad="60"/>
<connect gate="G$1" pin="AVDD@9" pad="65"/>
<connect gate="G$1" pin="D0" pad="8"/>
<connect gate="G$1" pin="D1" pad="7"/>
<connect gate="G$1" pin="D2" pad="6"/>
<connect gate="G$1" pin="D3" pad="5"/>
<connect gate="G$1" pin="D4" pad="4"/>
<connect gate="G$1" pin="D5" pad="3"/>
<connect gate="G$1" pin="D6" pad="2"/>
<connect gate="G$1" pin="D7" pad="1"/>
<connect gate="G$1" pin="DACBP" pad="55"/>
<connect gate="G$1" pin="DACREST" pad="56"/>
<connect gate="G$1" pin="DGND@1" pad="11"/>
<connect gate="G$1" pin="DGND@10" pad="78"/>
<connect gate="G$1" pin="DGND@2" pad="12"/>
<connect gate="G$1" pin="DGND@3" pad="26"/>
<connect gate="G$1" pin="DGND@4" pad="27"/>
<connect gate="G$1" pin="DGND@5" pad="28"/>
<connect gate="G$1" pin="DGND@6" pad="72"/>
<connect gate="G$1" pin="DGND@7" pad="75"/>
<connect gate="G$1" pin="DGND@8" pad="76"/>
<connect gate="G$1" pin="DGND@9" pad="77"/>
<connect gate="G$1" pin="DIFF_CLKENABLE" pad="64"/>
<connect gate="G$1" pin="DVDD@1" pad="9"/>
<connect gate="G$1" pin="DVDD@2" pad="10"/>
<connect gate="G$1" pin="DVDD@3" pad="23"/>
<connect gate="G$1" pin="DVDD@4" pad="24"/>
<connect gate="G$1" pin="DVDD@5" pad="25"/>
<connect gate="G$1" pin="DVDD@6" pad="73"/>
<connect gate="G$1" pin="DVDD@7" pad="74"/>
<connect gate="G$1" pin="DVDD@8" pad="79"/>
<connect gate="G$1" pin="DVDD@9" pad="80"/>
<connect gate="G$1" pin="FSK/BPSK/HOLD" pad="29"/>
<connect gate="G$1" pin="I/O_UD_CLK" pad="20"/>
<connect gate="G$1" pin="IOUT1" pad="48"/>
<connect gate="G$1" pin="IOUT2" pad="52"/>
<connect gate="G$1" pin="MASTER_RESET" pad="71"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="NC@2" pad="35"/>
<connect gate="G$1" pin="NC@3" pad="57"/>
<connect gate="G$1" pin="NC@4" pad="58"/>
<connect gate="G$1" pin="NC@5" pad="63"/>
<connect gate="G$1" pin="OSK" pad="30"/>
<connect gate="G$1" pin="PLLFILTER" pad="61"/>
<connect gate="G$1" pin="REFCLK" pad="69"/>
<connect gate="G$1" pin="S/P_SELECT" pad="70"/>
<connect gate="G$1" pin="VINN" pad="43"/>
<connect gate="G$1" pin="VINP" pad="42"/>
<connect gate="G$1" pin="VOUT" pad="36"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD9854ASTZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P1074"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD9912" prefix="IC">
<description>&lt;b&gt;1 GSPS Direct Digital Synthesizer with 14-Bit DAC&lt;/b&gt;&lt;p&gt;
Source:  http://www.analog.com/static/imported-files/data_sheets/AD9912.pdf</description>
<gates>
<gate name="G$1" symbol="AD9912"/>
</gates>
<devices>
<device name="" package="LFCSP64">
<connects>
<connect gate="G$1" pin="AVDD3@1" pad="14"/>
<connect gate="G$1" pin="AVDD3@2" pad="37"/>
<connect gate="G$1" pin="AVDD3@3" pad="46"/>
<connect gate="G$1" pin="AVDD3@4" pad="47"/>
<connect gate="G$1" pin="AVDD3@5" pad="49"/>
<connect gate="G$1" pin="AVDD@1" pad="11"/>
<connect gate="G$1" pin="AVDD@10" pad="42"/>
<connect gate="G$1" pin="AVDD@11" pad="44"/>
<connect gate="G$1" pin="AVDD@12" pad="45"/>
<connect gate="G$1" pin="AVDD@13" pad="53"/>
<connect gate="G$1" pin="AVDD@2" pad="19"/>
<connect gate="G$1" pin="AVDD@3" pad="23"/>
<connect gate="G$1" pin="AVDD@4" pad="24"/>
<connect gate="G$1" pin="AVDD@5" pad="25"/>
<connect gate="G$1" pin="AVDD@6" pad="26"/>
<connect gate="G$1" pin="AVDD@7" pad="29"/>
<connect gate="G$1" pin="AVDD@8" pad="30"/>
<connect gate="G$1" pin="AVDD@9" pad="36"/>
<connect gate="G$1" pin="AVSS@1" pad="33"/>
<connect gate="G$1" pin="AVSS@2" pad="39"/>
<connect gate="G$1" pin="AVSS@3" pad="43"/>
<connect gate="G$1" pin="AVSS@4" pad="52"/>
<connect gate="G$1" pin="CLKMODESEL" pad="32"/>
<connect gate="G$1" pin="CSB" pad="61"/>
<connect gate="G$1" pin="DAC_OUT" pad="50"/>
<connect gate="G$1" pin="DAC_OUTB" pad="51"/>
<connect gate="G$1" pin="DAC_RSET" pad="48"/>
<connect gate="G$1" pin="DVDD@1" pad="3"/>
<connect gate="G$1" pin="DVDD@2" pad="5"/>
<connect gate="G$1" pin="DVDD@3" pad="7"/>
<connect gate="G$1" pin="DVDD_I/O" pad="1"/>
<connect gate="G$1" pin="DVSS@1" pad="2"/>
<connect gate="G$1" pin="DVSS@2" pad="4"/>
<connect gate="G$1" pin="DVSS@3" pad="6"/>
<connect gate="G$1" pin="DVSS@4" pad="8"/>
<connect gate="G$1" pin="DVSS@5" pad="56"/>
<connect gate="G$1" pin="DVSS@6" pad="57"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="FDBK_IN" pad="41"/>
<connect gate="G$1" pin="FDBK_INB" pad="40"/>
<connect gate="G$1" pin="IO_UPDATE" pad="60"/>
<connect gate="G$1" pin="LOOP_FILTER" pad="31"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="13"/>
<connect gate="G$1" pin="NC@3" pad="15"/>
<connect gate="G$1" pin="NC@4" pad="16"/>
<connect gate="G$1" pin="NC@5" pad="17"/>
<connect gate="G$1" pin="NC@6" pad="18"/>
<connect gate="G$1" pin="NC@7" pad="20"/>
<connect gate="G$1" pin="NC@8" pad="21"/>
<connect gate="G$1" pin="NC@9" pad="22"/>
<connect gate="G$1" pin="OUT" pad="35"/>
<connect gate="G$1" pin="OUTB" pad="34"/>
<connect gate="G$1" pin="OUT_CMOS" pad="38"/>
<connect gate="G$1" pin="PWRDOWN" pad="58"/>
<connect gate="G$1" pin="RESET" pad="59"/>
<connect gate="G$1" pin="S1" pad="9"/>
<connect gate="G$1" pin="S2" pad="10"/>
<connect gate="G$1" pin="S3" pad="54"/>
<connect gate="G$1" pin="S4" pad="55"/>
<connect gate="G$1" pin="SCLK" pad="64"/>
<connect gate="G$1" pin="SDIO" pad="63"/>
<connect gate="G$1" pin="SDO" pad="62"/>
<connect gate="G$1" pin="SYSCLK" pad="27"/>
<connect gate="G$1" pin="SYSCLKB" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD9912BCPZ"/>
<attribute name="OC_FARNELL" value="1542712"/>
<attribute name="OC_NEWARK" value="61M3822"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC84*-52" prefix="IC">
<description>&lt;b&gt;ADuC845/ADuC847/ADuC848&lt;/b&gt; Package MQFP 52&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADUC845_847_848.pdf</description>
<gates>
<gate name="G$1" symbol="ADUC845-52"/>
</gates>
<devices>
<device name="" package="MQFP52">
<connects>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AINCOM/DAC" pad="13"/>
<connect gate="G$1" pin="ALE" pad="42"/>
<connect gate="G$1" pin="AVDD" pad="5"/>
<connect gate="G$1" pin="DAC" pad="14"/>
<connect gate="G$1" pin="DGND" pad="21"/>
<connect gate="G$1" pin="DGND@1" pad="35"/>
<connect gate="G$1" pin="DGND@2" pad="47"/>
<connect gate="G$1" pin="DVDD" pad="20"/>
<connect gate="G$1" pin="DVDD@1" pad="34"/>
<connect gate="G$1" pin="DVDD@2" pad="48"/>
<connect gate="G$1" pin="EA" pad="40"/>
<connect gate="G$1" pin="P0_0" pad="43"/>
<connect gate="G$1" pin="P0_1" pad="44"/>
<connect gate="G$1" pin="P0_2" pad="45"/>
<connect gate="G$1" pin="P0_3" pad="46"/>
<connect gate="G$1" pin="P0_4" pad="49"/>
<connect gate="G$1" pin="P0_5" pad="50"/>
<connect gate="G$1" pin="P0_6" pad="51"/>
<connect gate="G$1" pin="P0_7" pad="52"/>
<connect gate="G$1" pin="P1_0/AIN1" pad="1"/>
<connect gate="G$1" pin="P1_1/AIN2" pad="2"/>
<connect gate="G$1" pin="P1_2/AIN3/REFIN2+" pad="3"/>
<connect gate="G$1" pin="P1_3/AIN4/REFIN2-" pad="4"/>
<connect gate="G$1" pin="P1_4/AIN5" pad="9"/>
<connect gate="G$1" pin="P1_5/AIN6" pad="10"/>
<connect gate="G$1" pin="P1_6/AIN7/IEXC1" pad="11"/>
<connect gate="G$1" pin="P1_7/AIN8/IEXC2" pad="12"/>
<connect gate="G$1" pin="P2_0/SCLOCK_SPI" pad="28"/>
<connect gate="G$1" pin="P2_1/MOSI" pad="29"/>
<connect gate="G$1" pin="P2_2/MISO" pad="30"/>
<connect gate="G$1" pin="P2_3/SS/T2" pad="31"/>
<connect gate="G$1" pin="P2_4/T2EX" pad="36"/>
<connect gate="G$1" pin="P2_5/PWM0" pad="37"/>
<connect gate="G$1" pin="P2_6/PWM1" pad="38"/>
<connect gate="G$1" pin="P2_7/PWMCLK" pad="39"/>
<connect gate="G$1" pin="P3_0/RXD" pad="16"/>
<connect gate="G$1" pin="P3_1/TXD" pad="17"/>
<connect gate="G$1" pin="P3_2/INT0" pad="18"/>
<connect gate="G$1" pin="P3_3/INT1" pad="19"/>
<connect gate="G$1" pin="P3_4/T0" pad="22"/>
<connect gate="G$1" pin="P3_5/T1" pad="23"/>
<connect gate="G$1" pin="P3_6/WR" pad="24"/>
<connect gate="G$1" pin="P3_7/RD" pad="25"/>
<connect gate="G$1" pin="PSEN" pad="41"/>
<connect gate="G$1" pin="REFIN+" pad="8"/>
<connect gate="G$1" pin="REFIN-" pad="7"/>
<connect gate="G$1" pin="RESET" pad="15"/>
<connect gate="G$1" pin="SCLK_I2C" pad="26"/>
<connect gate="G$1" pin="SDATA" pad="27"/>
<connect gate="G$1" pin="XTAL1" pad="32"/>
<connect gate="G$1" pin="XTAL2" pad="33"/>
</connects>
<technologies>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC845BSZ62-5"/>
<attribute name="OC_FARNELL" value="1438809"/>
<attribute name="OC_NEWARK" value="15P0574"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC847BSZ62-3"/>
<attribute name="OC_FARNELL" value="1438810"/>
<attribute name="OC_NEWARK" value="15P0575"/>
</technology>
<technology name="8">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADUC848BSZ62-5"/>
<attribute name="OC_FARNELL" value="1438811"/>
<attribute name="OC_NEWARK" value="15P0578"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADUC84*-56" prefix="IC">
<description>&lt;b&gt;MicroConverter® Multichannel 24-/16-Bit ADCs with Embedded 62 kB Flash and Single-Cycle MCU&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/ADUC845_847_848.pdf</description>
<gates>
<gate name="G$1" symbol="ADUC845-56"/>
</gates>
<devices>
<device name="" package="LFCSP56">
<connects>
<connect gate="G$1" pin="AGND" pad="5"/>
<connect gate="G$1" pin="AGND@1" pad="6"/>
<connect gate="G$1" pin="AIN10" pad="16"/>
<connect gate="G$1" pin="AIN9" pad="15"/>
<connect gate="G$1" pin="AINCOM/DAC" pad="13"/>
<connect gate="G$1" pin="ALE" pad="45"/>
<connect gate="G$1" pin="AVDD" pad="4"/>
<connect gate="G$1" pin="DAC" pad="14"/>
<connect gate="G$1" pin="DGND" pad="23"/>
<connect gate="G$1" pin="DGND@1" pad="37"/>
<connect gate="G$1" pin="DGND@2" pad="38"/>
<connect gate="G$1" pin="DGND@3" pad="50"/>
<connect gate="G$1" pin="DVDD" pad="22"/>
<connect gate="G$1" pin="DVDD@1" pad="36"/>
<connect gate="G$1" pin="DVDD@2" pad="51"/>
<connect gate="G$1" pin="EA" pad="43"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="P0_0" pad="46"/>
<connect gate="G$1" pin="P0_1" pad="47"/>
<connect gate="G$1" pin="P0_2" pad="48"/>
<connect gate="G$1" pin="P0_3" pad="49"/>
<connect gate="G$1" pin="P0_4" pad="52"/>
<connect gate="G$1" pin="P0_5" pad="53"/>
<connect gate="G$1" pin="P0_6" pad="54"/>
<connect gate="G$1" pin="P0_7" pad="55"/>
<connect gate="G$1" pin="P1_0/AIN1" pad="56"/>
<connect gate="G$1" pin="P1_1/AIN2" pad="1"/>
<connect gate="G$1" pin="P1_2/AIN3/REFIN2+" pad="2"/>
<connect gate="G$1" pin="P1_3/AIN4/REFIN2-" pad="3"/>
<connect gate="G$1" pin="P1_4/AIN5" pad="9"/>
<connect gate="G$1" pin="P1_5/AIN6" pad="10"/>
<connect gate="G$1" pin="P1_6/AIN7/IEXC1" pad="11"/>
<connect gate="G$1" pin="P1_7/AIN8/IEXC2" pad="12"/>
<connect gate="G$1" pin="P2_0/SCLOCK_SPI" pad="30"/>
<connect gate="G$1" pin="P2_1/MOSI" pad="31"/>
<connect gate="G$1" pin="P2_2/MISO" pad="32"/>
<connect gate="G$1" pin="P2_3/SS/T2" pad="33"/>
<connect gate="G$1" pin="P2_4/T2EX" pad="39"/>
<connect gate="G$1" pin="P2_5/PWM0" pad="40"/>
<connect gate="G$1" pin="P2_6/PWM1" pad="41"/>
<connect gate="G$1" pin="P2_7/PWMCLK" pad="42"/>
<connect gate="G$1" pin="P3_0/RXD" pad="18"/>
<connect gate="G$1" pin="P3_1/TXD" pad="19"/>
<connect gate="G$1" pin="P3_2/INT0" pad="20"/>
<connect gate="G$1" pin="P3_3/INT1" pad="21"/>
<connect gate="G$1" pin="P3_4/T0" pad="24"/>
<connect gate="G$1" pin="P3_5/T1" pad="25"/>
<connect gate="G$1" pin="P3_6/WR" pad="26"/>
<connect gate="G$1" pin="P3_7/RD" pad="27"/>
<connect gate="G$1" pin="PSEN" pad="44"/>
<connect gate="G$1" pin="REFIN+" pad="8"/>
<connect gate="G$1" pin="REFIN-" pad="7"/>
<connect gate="G$1" pin="RESET" pad="17"/>
<connect gate="G$1" pin="SCLK_I2C" pad="28"/>
<connect gate="G$1" pin="SDATA" pad="29"/>
<connect gate="G$1" pin="XTAL1" pad="34"/>
<connect gate="G$1" pin="XTAL2" pad="35"/>
</connects>
<technologies>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
