<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.1">
<drawing>
<library>
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="DIL20">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
<package name="S44">
<description>&lt;B&gt;Throughhole Plastic J-Leaded Chip Carrier Socket&lt;/B&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;B&gt;Plastic J-Leaded Chip Carrier&lt;/B&gt;</description>
</package>
<package name="PLCC-SM44">
<description>&lt;B&gt;SMD Plastic J-Leaded Chip Carrier Socket&lt;/B&gt;</description>
</package>
<package name="SSOP20D8">
<description>&lt;B&gt;Plastic Shrink Small Outline Package&lt;/B&gt;</description>
</package>
<package name="SOIC8">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="SO20L">
<description>&lt;B&gt;Small Outline Package&lt;/B&gt; SOIC 0.300"</description>
</package>
<package name="TQFP48">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="SOIC20S">
<description>&lt;B&gt;Wide Plastic Gull Wing Small Outline Package&lt;/B&gt;</description>
</package>
<package name="LOGO">
<description>&lt;B&gt;Logo&lt;/B&gt;</description>
</package>
<package name="PQFP44">
<description>&lt;B&gt;Plastic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="PLCC32R">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
rectangle</description>
</package>
<package name="TSOP32">
<description>&lt;b&gt;TSOP32&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
<package name="DIL32">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO32X">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
extra wide body 8.9 mm/JEDEC MO-120AC</description>
</package>
<package name="MSOP8">
<description>&lt;b&gt;8M, 8-Lead, 0.118" Wide, Miniature Small Outline Package&lt;/b&gt;&lt;p&gt;
MSOP&lt;br&gt;
8M-Package doc1097.pdf</description>
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="PSSO20">
<description>&lt;b&gt;PSSO20&lt;/b&gt;</description>
</package>
<package name="TQFP144">
<description>&lt;b&gt;QFP144&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square (smd-ipc)</description>
</package>
<package name="PLCC52">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="SSOP24">
<description>&lt;b&gt; SSOP 24&lt;/b&gt;&lt;p&gt;
Source: Uploaded by Heiko Künzel &lt;heiko.kuenzel@atg-gera.de&gt; from ATG Automatisierungstechnik Gera&lt;br&gt;
Mon Mar 10 13:32:48 2003 Atmel-Library mit zusätzlich T83C5121-Prozessor im SSOP24-Package.&lt;br&gt;
Package centre and &amp;lt;NAME &amp; &amp;lt;VALUE placed by librarian@cadsoft.de.</description>
</package>
<package name="PLCC84">
<description>&lt;b&gt;Plastic J-Lead Chip Carrier&lt;/b&gt;</description>
</package>
<package name="TQFP80">
<description>&lt;b&gt;TQFP 80&lt;/b&gt; thin quad flat pack&lt;p&gt;
Source: www.atmwel.com .. doc4109.pdf</description>
</package>
<package name="BGA81">
<description>&lt;b&gt;Ball Grid Array&lt;/b&gt; 81 leads&lt;p&gt;
Source: www.atmwel.com .. doc4109.pdf</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AB&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="SO24W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MO-119AA&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="PLCC28">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="VQFP32">
<description>&lt;b&gt;Quad Flat Pack&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.pdf</description>
</package>
<package name="LFBGA256_A_291X326">
<description>Auto generated by &lt;b&gt;make-symbol-device-package(bsdl).ulp&lt;/b&gt;&lt;p&gt;Source: at91rm9200_bga.bsd</description>
</package>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="PLCC20">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;</description>
</package>
<package name="MLF64">
<description>&lt;b&gt;64M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="TQFP64">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;&lt;p&gt;
Updated from atml.lbr 17.01.2005 alf@cadsoft.de</description>
</package>
<package name="VQFP64">
<description>&lt;b&gt;64-lead VQVP&lt;/b&gt;&lt;p&gt;
Source. http://www.atmel.com/dyn/resources/prod_documents/doc4136.pdf</description>
</package>
<package name="MLF64-TH">
<description>&lt;b&gt;64M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF32-TH">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF16-TH">
<description>&lt;b&gt;HP-VFQFP-N16&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF20-5X5-TH">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; QFN 20  -5  x 5 mm Micro Lead Frame package (MLF)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4533.pdf</description>
</package>
<package name="MLF16">
<description>&lt;b&gt;HP-VFQFP-N16&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF20-5X5">
<description>&lt;b&gt;HP-VFQFP-N20&lt;/b&gt; 5 x 5 mm Micro Lead Frame package (MLF)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4533.pdf</description>
</package>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="MLF44">
<description>&lt;b&gt;44M1&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
<package name="QFN44ML8X8">
<description>&lt;b&gt;44-Lead Plastic Quad Flat No Lead Package (ML)&lt;/b&gt; 8x8 mm Body (QFN)&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
</package>
<package name="LQFP100">
<description>&lt;b&gt;LQFP 100&lt;/b&gt;&lt;p&gt;
Source: 6120s.pdf</description>
</package>
<package name="TFBGA100">
<description>&lt;b&gt;TFBGA 100&lt;/b&gt;&lt;p&gt;
Source: 6120s.pdf</description>
</package>
<package name="TSSOP8">
<description>&lt;b&gt;8A2-TSSOP&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc5089.pdf</description>
</package>
<package name="10M1">
<description>&lt;b&gt;10M1&lt;/b&gt; 10-pad, 3 x 3 x 1.0 mm Body&lt;p&gt;
Lead Pitch 0.50 mm, 1.64 x 2.60 mm Exposed Pad, Micro Lead Frame Package&lt;br&gt;
MLF10, QFN10&lt;/b&gt;&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
<package name="8S2">
<description>&lt;b&gt;8S2&lt;/b&gt; 8-lead, 0.208 Body&lt;p&gt;
Plastic Small Outline Package (EIAJ)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
<package name="8S1">
<description>&lt;b&gt;8S1&lt;/b&gt; 8-lead (0.150" Wide Body)&lt;p&gt;
Plastic Gull Wing Small Outline (JEDEC SOIC)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
<package name="20M1">
<description>&lt;b&gt;20M1&lt;/b&gt; 20-pad, 4 x 4 x 0.8 mm Body&lt;p&gt;
Lead Pitch 0.50 mm, 2.6 mm Exposed Pad, Micro Lead Frame Package (MLF)&lt;br&gt;

Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;44-lead Thin Quad Flat Package&lt;/b&gt;</description>
</package>
<package name="MLF44-TH">
<description>&lt;b&gt;44M1&lt;/b&gt; Micro Lead Frame package (MLF)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2593.pdf</description>
</package>
<package name="TQFP100">
<description>&lt;b&gt;100-lead Thin Quad Flat Pack Package&lt;/b&gt;</description>
</package>
<package name="64M1">
<description>&lt;b&gt;64M1&lt;/b&gt;&lt;p&gt; 64-pad, 9 x 9 x 1.0 mm&lt;p&gt;
 Lead Pitch 0.50 mm, 5.40 mm Exposed Pad, Micro Lead Frame Package (MLF)&lt;br&gt;
Source: http://www.atmel.com .. doc8023.pdf</description>
</package>
<package name="28T-TSOP-1">
<description>&lt;b&gt;28T&lt;/b&gt; 28-lead (8 x 13.4 mm) Plastic Thin Small Outline Type I (TSOP)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc3542.pdf</description>
</package>
<package name="VDFN-8">
<description>&lt;b&gt;8M1-A-MLF (VDFN)&lt;/b&gt; 6 x 5 mm&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc3500.pdf</description>
</package>
<package name="MLF20-4X4">
<description>&lt;b&gt;20M1&lt;/b&gt; 20-pad, 4 x 4 x 0.8 mm Body&lt;p&gt;
Lead Pitch 0.50 mm, 2.6 mm Exposed Pad, Micro Lead Frame Package (MLF)&lt;br&gt;
Source: &lt;a href="http://www.atmel.com/Images/doc2543.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
<symbols>
<symbol name="6-I/O-1">
<pin name="(XTAL2)PB4"/>
<pin name="(XTAL1)PB3"/>
<pin name="(RESET)PB5"/>
<pin name="(T0)PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="6-I/O-2">
<pin name="(XTAL2)PB4"/>
<pin name="(XTAL1)PB3"/>
<pin name="(RESET)PB5"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="5-I/O-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PB4"/>
<pin name="(CLOCK)PB3"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
</symbol>
<symbol name="6-I/O-3">
<pin name="(ADC3)PB4"/>
<pin name="(ADC2)PB3"/>
<pin name="(ADC0)PB5"/>
<pin name="(ADC1)PB2"/>
<pin name="(OCP)PB1"/>
<pin name="(AREF)PB0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="16-I/O-1">
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="(ADC3)PB4"/>
<pin name="(ADC2)PB3"/>
<pin name="(ADC1)PB2"/>
<pin name="(OCP)PB1"/>
<pin name="(AVREF)PB0"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PC7"/>
<pin name="(ADC0)PB5"/>
</symbol>
<symbol name="15-I/O-1">
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="PB4"/>
<pin name="PB3"/>
<pin name="PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="(T0)PD4"/>
<pin name="PD3"/>
<pin name="(INT0)PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" function="dot"/>
</symbol>
<symbol name="3-I/O-1">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="(SCK)PB2"/>
<pin name="(MISO)PB1"/>
<pin name="(MOSI)PB0"/>
</symbol>
<symbol name="20-I/O-1">
<pin name="(ADC5)PC5"/>
<pin name="(ADC4)PC4"/>
<pin name="(ADC3)PC3"/>
<pin name="(ADC2)PC2"/>
<pin name="(ADC1)PC1"/>
<pin name="(ADC0)PC0"/>
<pin name="(SCK)PB5"/>
<pin name="(MISO)PB4"/>
<pin name="(MOSI)PB3"/>
<pin name="(SS)PB2"/>
<pin name="(OC1)PB1"/>
<pin name="(ICP)PB0"/>
<pin name="(AIN1)PD7"/>
<pin name="(AIN0)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
<pin name="NC4" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="32-I/O-1">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="OC1B"/>
<pin name="ALE"/>
<pin name="ICP"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
</symbol>
<symbol name="32-I/O-2">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="OC1B"/>
<pin name="ALE"/>
<pin name="ICP"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="48-I/O-1">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4)" direction="in"/>
<pin name="PF5(ADC5)" direction="in"/>
<pin name="PF6(ADC6)" direction="in"/>
<pin name="PF7(ADC7)" direction="in"/>
<pin name="(RXD)PE0"/>
<pin name="(TXD)PE1"/>
<pin name="(AC+)PE2"/>
<pin name="(AC-)PE3"/>
<pin name="(INT4)PE4"/>
<pin name="(INT5)PE5"/>
<pin name="(INT6)PE6"/>
<pin name="(INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(INT3)PD3"/>
<pin name="(INT2)PD2"/>
<pin name="(INT1)PD1"/>
<pin name="(INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TOSC2"/>
<pin name="TOSC1"/>
<pin name="WR" function="dot"/>
<pin name="RD" function="dot"/>
<pin name="ALE"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="15-I/O-2">
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="PB4"/>
<pin name="(OCI)PB3"/>
<pin name="PB2"/>
<pin name="(AIN1)PB1"/>
<pin name="(AIN0)PB0"/>
<pin name="(ICP)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" function="dot"/>
</symbol>
<symbol name="20-I/O-2">
<pin name="(ADC5)PC5"/>
<pin name="(ADC4)PC4"/>
<pin name="(ADC3)PC3"/>
<pin name="(ADC2)PC2"/>
<pin name="(ADC1)PC1"/>
<pin name="(ADC0)PC0)"/>
<pin name="(SCK)PB5"/>
<pin name="(MISO)PB4"/>
<pin name="(MOSI)PB3"/>
<pin name="(SS)PB2"/>
<pin name="(OC1)PB1"/>
<pin name="(ICP)PB0"/>
<pin name="(AIN1)PD7"/>
<pin name="(AIN0)PD6"/>
<pin name="(T1)PD5"/>
<pin name="(T0)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD)PD1"/>
<pin name="(RXD)PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-3">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-4">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="15-I/O-3">
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="INT1" direction="in"/>
<pin name="INT0" direction="in"/>
<pin name="AVCC" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="ADIN5" direction="in"/>
<pin name="ADIN4" direction="in"/>
<pin name="ADIN3" direction="in"/>
<pin name="ADIN2" direction="in"/>
<pin name="ADIN1" direction="in"/>
<pin name="ADIN0" direction="in"/>
<pin name="NC13" direction="nc"/>
<pin name="NC12" direction="nc"/>
<pin name="NC11" direction="nc"/>
<pin name="NC10" direction="nc"/>
<pin name="NC9" direction="nc"/>
<pin name="NC8" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="NC6" direction="nc"/>
<pin name="NC5" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC14" direction="nc"/>
<pin name="NC15" direction="nc"/>
<pin name="NC16" direction="nc"/>
<pin name="NC17" direction="nc"/>
<pin name="NC18" direction="nc"/>
<pin name="NC19" direction="nc"/>
<pin name="NC20" direction="nc"/>
<pin name="NC21" direction="nc"/>
<pin name="NC22" direction="nc"/>
<pin name="NC23" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="NC24" direction="nc"/>
<pin name="NC25" direction="nc"/>
<pin name="NC26" direction="nc"/>
</symbol>
<symbol name="35-I/O-1">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(TXD1)PB3"/>
<pin name="(RXD1)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(RD)PD7"/>
<pin name="(WR)PD6"/>
<pin name="(TOSC2)PD5"/>
<pin name="(TOSC1)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD0)PD1"/>
<pin name="(RXD0)PD0"/>
<pin name="(OC1B)PE2"/>
<pin name="(ALE)PE1"/>
<pin name="(INT2)PE0"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="in"/>
</symbol>
<symbol name="35-I/O-2">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(TXD1)PB3"/>
<pin name="(RXD1)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="(RD)PD7"/>
<pin name="(WR)PD6"/>
<pin name="(TOSC2)PD5"/>
<pin name="(TOSC1)PD4"/>
<pin name="(INT1)PD3"/>
<pin name="(INT0)PD2"/>
<pin name="(TXD0)PD1"/>
<pin name="(RXD0)PD0"/>
<pin name="(OC1B)PE2"/>
<pin name="(ALE)PE1"/>
<pin name="(INT2)PE0"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="32-I/O-5">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-6">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="20-I/O-3">
<pin name="PB5" direction="in"/>
<pin name="PB4(INT1)" direction="in"/>
<pin name="PB3(INT0)" direction="in"/>
<pin name="PB2(T0)" direction="in"/>
<pin name="PB1(AIN1)" direction="in"/>
<pin name="PB0(AIN0)" direction="in"/>
<pin name="PA3"/>
<pin name="(IR)PA2" direction="out"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="PB7" direction="in"/>
<pin name="PB6" direction="in"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC1" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="20-I/O-4">
<pin name="PB5" direction="in"/>
<pin name="PB4(INT1)" direction="in"/>
<pin name="PB3(INT0)" direction="in"/>
<pin name="PB2(T0)" direction="in"/>
<pin name="PB1(AIN1)" direction="in"/>
<pin name="PB0(AIN0)" direction="in"/>
<pin name="PA3"/>
<pin name="(IR)PA2" direction="out"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="PB7" direction="in"/>
<pin name="PB6" direction="in"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="VCC1" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="NC5" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC1" direction="nc"/>
</symbol>
<symbol name="24CXX">
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="250X0">
<pin name="HOLD/" direction="in"/>
<pin name="CS/" direction="in"/>
<pin name="SO" direction="in"/>
<pin name="WP/" direction="in"/>
<pin name="SCK"/>
<pin name="SI"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="SDE2506">
<pin name="CLK" direction="in"/>
<pin name="CE/" direction="in"/>
<pin name="D"/>
<pin name="NC" direction="nc"/>
<pin name="TP" direction="in"/>
<pin name="TG"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="93CX6">
<pin name="DO" direction="out"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SK"/>
<pin name="ORG" direction="in"/>
<pin name="DC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="15IO-1">
<pin name="AIN0-PB0"/>
<pin name="AIN1-PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="MOSI-PB5"/>
<pin name="MISO-PB6"/>
<pin name="SCK-PB7"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="INT0-PD2"/>
<pin name="PD3"/>
<pin name="T0-PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="RST/"/>
</symbol>
<symbol name="5IO-1">
<pin name="MOSI-PB0"/>
<pin name="MISO-PB1"/>
<pin name="SCK-PB2"/>
<pin name="CLK-PB3"/>
<pin name="PB4"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="RST/"/>
</symbol>
<symbol name="32IO-1">
<pin name="AD7-PA7"/>
<pin name="AD6-PA6"/>
<pin name="AD5-PA5"/>
<pin name="AD4-PA4"/>
<pin name="AD3-PA3"/>
<pin name="AD2-PA2"/>
<pin name="AD1-PA1"/>
<pin name="AD0-PA0"/>
<pin name="A15-PC7"/>
<pin name="A14-PC6"/>
<pin name="A13-PC5"/>
<pin name="A12-PC4"/>
<pin name="A11-PC3"/>
<pin name="A10-PC2"/>
<pin name="A9-PC1"/>
<pin name="A8-PC0"/>
<pin name="PB7-SCK"/>
<pin name="PB6-MISO"/>
<pin name="PB5-MOSI"/>
<pin name="PB4-SS/"/>
<pin name="PB3-AIN1"/>
<pin name="PB2-AIN0"/>
<pin name="PB1-T1"/>
<pin name="PB0-T0"/>
<pin name="PD0-RXD"/>
<pin name="PD1-TXD"/>
<pin name="PD2-INT0"/>
<pin name="PD3-INT1"/>
<pin name="PD4"/>
<pin name="PD5-OC1A"/>
<pin name="PD6-WR/"/>
<pin name="PD7-RD/"/>
<pin name="XTAL2"/>
<pin name="XTAL1"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RST/" direction="in"/>
<pin name="ICP"/>
<pin name="ALE"/>
<pin name="OC1B"/>
</symbol>
<symbol name="89C2051">
<pin name="P3.7"/>
<pin name="P3.5-T1"/>
<pin name="P3.4-T0"/>
<pin name="P3.3-INT1/"/>
<pin name="P3.2-INTO/"/>
<pin name="P3.1-TXD"/>
<pin name="P3.0-RXD"/>
<pin name="P1.7"/>
<pin name="P1.6"/>
<pin name="P1.5"/>
<pin name="P1.4"/>
<pin name="P1.3"/>
<pin name="P1.2"/>
<pin name="AIN1-P1.1"/>
<pin name="AIN0-P1.0"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RST-VPP" direction="in"/>
</symbol>
<symbol name="48-I/O-2">
<pin name="ADC0-PF0" direction="in"/>
<pin name="ADC1-PF1" direction="in"/>
<pin name="ADC2-PF2" direction="in"/>
<pin name="ADC3-PF3" direction="in"/>
<pin name="ADC4-PF4" direction="in"/>
<pin name="ADC5-PF5" direction="in"/>
<pin name="ADC6-PF6" direction="in"/>
<pin name="ADC7-PF7" direction="in"/>
<pin name="RXD-PE0" direction="out"/>
<pin name="TXD-PE1" direction="out"/>
<pin name="AC+_PE2" direction="out"/>
<pin name="AC-_PE3" direction="out"/>
<pin name="INT4-PE4" direction="out"/>
<pin name="INT5-PE5" direction="out"/>
<pin name="INT6-PE6" direction="out"/>
<pin name="INT7-PE7" direction="out"/>
<pin name="PD7-T2"/>
<pin name="PD6-T1"/>
<pin name="PD5"/>
<pin name="PD4-IC1"/>
<pin name="PD3-INT3"/>
<pin name="PD2-INT2"/>
<pin name="PD1-INT1"/>
<pin name="PD0-INT0"/>
<pin name="A15-PC7"/>
<pin name="A14-PC6"/>
<pin name="A13-PC5"/>
<pin name="A12-PC4"/>
<pin name="A11-PC3"/>
<pin name="A10-PC2"/>
<pin name="A9-PC1"/>
<pin name="A8-PC0"/>
<pin name="OC2-PB7"/>
<pin name="OC1B-PB6"/>
<pin name="OC1A-PB5"/>
<pin name="OC0-PB4"/>
<pin name="MISO-PB3"/>
<pin name="MOSI-PB2"/>
<pin name="SCK-PB1"/>
<pin name="SS-PB0"/>
<pin name="AD6-PA6"/>
<pin name="AD7-PA7"/>
<pin name="AD5-PA5"/>
<pin name="AD4-PA4"/>
<pin name="AD3-PA3"/>
<pin name="AD2-PA2"/>
<pin name="AD1-PA1"/>
<pin name="AD0-PA0"/>
<pin name="AVCC"/>
<pin name="AGND"/>
<pin name="AVREF"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="01" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="02" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TOSC2"/>
<pin name="TOSC1"/>
<pin name="WR/"/>
<pin name="RD/"/>
<pin name="ALE"/>
<pin name="RESET/" direction="in"/>
<pin name="PEN/" direction="in"/>
</symbol>
<symbol name="AT89C52">
<pin name="EA" direction="in"/>
<pin name="P0.0AD0"/>
<pin name="P0.1AD1"/>
<pin name="P0.2AD2"/>
<pin name="P0.3AD3"/>
<pin name="P0.4AD4"/>
<pin name="P0.5AD5"/>
<pin name="P0.6AD6"/>
<pin name="P0.7AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0_T2"/>
<pin name="P1.1_T2EX"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR"/>
<pin name="P3.7/RD"/>
</symbol>
<symbol name="VCCGND">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="27C080">
<pin name="A16" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="O0" direction="hiz"/>
<pin name="O1" direction="hiz"/>
<pin name="O2" direction="hiz"/>
<pin name="O3" direction="hiz"/>
<pin name="O4" direction="hiz"/>
<pin name="O5" direction="hiz"/>
<pin name="O6" direction="hiz"/>
<pin name="O7" direction="hiz"/>
<pin name="!CE" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="!OE!VPP" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
</symbol>
<symbol name="AT91R4008">
<pin name="NCS0" direction="out"/>
<pin name="NCS1" direction="out"/>
<pin name="NWAIT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="NWDOVF" direction="out"/>
<pin name="MCKI" direction="in"/>
<pin name="NRW0/NWE" direction="out"/>
<pin name="NRD/NOE" direction="out"/>
<pin name="NRW1/NUB" direction="out"/>
<pin name="NRST" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
</symbol>
<symbol name="ICE-TEST">
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TDI" direction="in"/>
<pin name="TCK" direction="in"/>
</symbol>
<symbol name="AT91R4008-PARPORT">
<pin name="P0/TCLK0"/>
<pin name="P1/TIOA0"/>
<pin name="P2/TIOB0"/>
<pin name="P3/TCLK1"/>
<pin name="P4/TIOA1"/>
<pin name="P5/TIOB1"/>
<pin name="P6/TCLK2"/>
<pin name="P7/TIOA2"/>
<pin name="P8/TIOB2"/>
<pin name="P9/IRQ0"/>
<pin name="P10/IRQ1"/>
<pin name="P11/IRQ2"/>
<pin name="P12/FIQ"/>
<pin name="P13/SCK0"/>
<pin name="P14/TXD0"/>
<pin name="P15/RXD0"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="P18"/>
<pin name="P19"/>
<pin name="P20/SCK1"/>
<pin name="P21/TXD1/NTRI"/>
<pin name="P22/RXD1"/>
<pin name="P23"/>
<pin name="P24/BMS"/>
<pin name="P25/MCKO"/>
<pin name="P26/NCS2"/>
<pin name="P27/NCS3"/>
</symbol>
<symbol name="AT91R4008-ADR">
<pin name="P31/CS4/A23" direction="out"/>
<pin name="P30/CS5/A22" direction="out"/>
<pin name="P29/CS6/A21" direction="out"/>
<pin name="P28/CS7/A20" direction="out"/>
<pin name="NLB/A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
</symbol>
<symbol name="D0-32">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
<pin name="D16" direction="hiz"/>
<pin name="D17" direction="hiz"/>
<pin name="D18" direction="hiz"/>
<pin name="D19" direction="hiz"/>
<pin name="D20" direction="hiz"/>
<pin name="D21" direction="hiz"/>
<pin name="D22" direction="hiz"/>
<pin name="D23" direction="hiz"/>
<pin name="D24" direction="hiz"/>
<pin name="D25" direction="hiz"/>
<pin name="D26" direction="hiz"/>
<pin name="D27" direction="hiz"/>
<pin name="D28" direction="hiz"/>
<pin name="D29" direction="hiz"/>
<pin name="D30" direction="hiz"/>
<pin name="D31" direction="hiz"/>
</symbol>
<symbol name="D0-15">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="VDDIO">
<pin name="VDDIO" direction="pwr"/>
</symbol>
<symbol name="VDDCORE">
<pin name="VDDCORE" direction="pwr"/>
</symbol>
<symbol name="TINY26">
<pin name="(ADC8/XTAL2)PB5"/>
<pin name="(ADC7/XTAL1)PB4"/>
<pin name="(OC1B)PB3"/>
<pin name="(SCK/SCL/!OC1B!)PB2"/>
<pin name="(MISO/DO/OC1A)PB1"/>
<pin name="(MOSI/DI/SDA/!OC1A!)PB0"/>
<pin name="(ADC6/AIN1)PA7"/>
<pin name="(ADC5/AIN0)PA6"/>
<pin name="(ADC4)PA5"/>
<pin name="(ADC3)PA4"/>
<pin name="(AREF)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="(ADC10/!RESET!)PB7"/>
<pin name="(ADC9/INT0/T0)PB6"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="SAM9708">
<pin name="READY" direction="hiz"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="IRQ" direction="hiz"/>
<pin name="!CS" direction="in"/>
<pin name="OVCK-OUT" direction="out"/>
<pin name="X1" direction="out"/>
<pin name="X2" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="LDTEST" direction="in"/>
<pin name="!PWDN" direction="in"/>
<pin name="!IO16" direction="hiz"/>
<pin name="!RAS"/>
<pin name="!CAS"/>
<pin name="!REFRESH"/>
<pin name="RBS" direction="out"/>
<pin name="CK_OUT" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
</symbol>
<symbol name="WD15">
<pin name="WD0"/>
<pin name="WD1"/>
<pin name="WD2"/>
<pin name="WD3"/>
<pin name="WD4"/>
<pin name="WD5"/>
<pin name="WD6"/>
<pin name="WD7"/>
<pin name="WD8"/>
<pin name="WD9"/>
<pin name="WD10"/>
<pin name="WD11"/>
<pin name="WD12"/>
<pin name="WD13"/>
<pin name="WD14"/>
<pin name="WD15"/>
</symbol>
<symbol name="WA27">
<pin name="WA0" direction="out"/>
<pin name="WA1" direction="out"/>
<pin name="WA2" direction="out"/>
<pin name="WA3" direction="out"/>
<pin name="WA4" direction="out"/>
<pin name="WA5" direction="out"/>
<pin name="WA6" direction="out"/>
<pin name="WA7" direction="out"/>
<pin name="WA8" direction="out"/>
<pin name="WA9" direction="out"/>
<pin name="WA10" direction="out"/>
<pin name="WA11" direction="out"/>
<pin name="WA12" direction="out"/>
<pin name="WA13" direction="out"/>
<pin name="WA14" direction="out"/>
<pin name="WA15" direction="out"/>
<pin name="WA16" direction="out"/>
<pin name="WA17" direction="out"/>
<pin name="WA18" direction="out"/>
<pin name="WA19" direction="out"/>
<pin name="WA20" direction="out"/>
<pin name="WA21" direction="out"/>
<pin name="WA22" direction="out"/>
<pin name="WA23" direction="out"/>
<pin name="WA24" direction="out"/>
<pin name="WA25" direction="out"/>
<pin name="WA26" direction="out"/>
</symbol>
<symbol name="SAM9708-SND">
<pin name="MIDI1_OUT" direction="in"/>
<pin name="MIDI2_OUT" direction="in"/>
<pin name="MIDI1_IN" direction="in"/>
<pin name="MIDI2_IN" direction="in"/>
<pin name="SD-IN0"/>
<pin name="SD-IN1"/>
<pin name="SD-IN2"/>
<pin name="SD-IN3"/>
<pin name="SD-OUT0" direction="out"/>
<pin name="SD-OUT1" direction="out"/>
<pin name="SD-OUT2" direction="out"/>
<pin name="SD-OUT3" direction="out"/>
<pin name="WS-OUT" direction="out"/>
<pin name="BCK-OUT" direction="out"/>
<pin name="SD-IN4"/>
<pin name="SD-IN5"/>
<pin name="SD-IN6"/>
<pin name="SD-IN7"/>
<pin name="SD-OUT4" direction="out"/>
<pin name="SD-OUT5" direction="out"/>
<pin name="SD-OUT6" direction="out"/>
<pin name="SD-OUT7" direction="out"/>
<pin name="LFT" direction="pas"/>
<pin name="!WCS0" direction="out"/>
<pin name="!WCS1" direction="out"/>
<pin name="!WWE" direction="out"/>
<pin name="!WOE" direction="out"/>
</symbol>
<symbol name="VCC1">
<pin name="VCC1" direction="pwr"/>
</symbol>
<symbol name="VCC2">
<pin name="VCC2" direction="pwr"/>
</symbol>
<symbol name="VC3">
<pin name="VC3" direction="pwr"/>
</symbol>
<symbol name="T8XC5121">
<pin name="CVSS" direction="pwr"/>
<pin name="LI" direction="pwr"/>
<pin name="CVCC" direction="pwr"/>
<pin name="P1.5/CRST"/>
<pin name="P1.4/CCLK"/>
<pin name="P1.3/CC4"/>
<pin name="P1.2/CPRES"/>
<pin name="P1.1/CC8"/>
<pin name="P1.0/CIO"/>
<pin name="RST"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="out"/>
<pin name="P3.7/CRST1/LED1"/>
<pin name="P3.6/CCLK1/LED0"/>
<pin name="P3.5/CIO1"/>
<pin name="P3.2/INT0"/>
<pin name="P3.4/T0"/>
<pin name="P3.3/INT1"/>
<pin name="P3.1/TXD"/>
<pin name="P3.0/RXD"/>
<pin name="VSS" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="EVCC" direction="pas"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="T8X5121-PLCC52">
<pin name="CVSS" direction="pwr"/>
<pin name="LI" direction="pwr"/>
<pin name="CVCC" direction="pwr"/>
<pin name="P1.5/CRST"/>
<pin name="P1.4/CCLK"/>
<pin name="P1.3/CC4"/>
<pin name="P1.2/CPRES"/>
<pin name="P1.1/CC8"/>
<pin name="P1.0/CIO"/>
<pin name="!RST"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTAL1" direction="out"/>
<pin name="P3.7/CRST1/LED1"/>
<pin name="P3.6/CCLK1/LED0"/>
<pin name="P3.5/CIO1"/>
<pin name="P3.2/INT0"/>
<pin name="P3.4/T0"/>
<pin name="P3.3/INT1"/>
<pin name="P3.1/TXD"/>
<pin name="P3.0/RXD"/>
<pin name="VSS" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="EVCC" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="EA"/>
<pin name="PSEN"/>
<pin name="ALE"/>
<pin name="P2.7/A15"/>
<pin name="P2.6/A14"/>
<pin name="P2.5/A13"/>
<pin name="P2.4/A12"/>
<pin name="P0.5/AD5"/>
<pin name="P2.3/A11"/>
<pin name="P2.2/A10"/>
<pin name="P2.1/A9"/>
<pin name="P2.0/A8"/>
<pin name="P0.7/AD7"/>
<pin name="P0.4/AD4"/>
<pin name="P0.6/AD6"/>
<pin name="P0.1/AD1"/>
<pin name="P0.2/AD2"/>
<pin name="P0.3/AD3"/>
<pin name="P0.0/AD0"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
</symbol>
<symbol name="AT89C51SND1C">
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AREFN" direction="in"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="P3.1/TXD"/>
<pin name="P3.0/RXD"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P4.3/!SS" direction="in"/>
<pin name="P4.0/MISO" direction="in"/>
<pin name="P4.1/MOSI" direction="out"/>
<pin name="P4.2/SCK" direction="out"/>
<pin name="P1.6/SCL"/>
<pin name="P1.7/SDA"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="FILT" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="out"/>
<pin name="RST" direction="in"/>
<pin name="!ISP" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="DCLK" direction="out"/>
<pin name="DESL" direction="out"/>
<pin name="SCLK" direction="out"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="MCLK" direction="out"/>
<pin name="MDAT"/>
<pin name="MCMD"/>
<pin name="P1.0/KIN0"/>
<pin name="P1.1/KIN1"/>
<pin name="P1.2/KIN2"/>
<pin name="P1.3/KIN3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.1"/>
<pin name="P5.0"/>
<pin name="P0.0/AD0"/>
<pin name="P0.1/AD1"/>
<pin name="P0.2/AD2"/>
<pin name="P0.3/AD3"/>
<pin name="P0.4/AD4"/>
<pin name="P0.5/AD5"/>
<pin name="P0.6/AD6"/>
<pin name="P0.7/AD7"/>
<pin name="P2.0/A8"/>
<pin name="P2.1/A9"/>
<pin name="P2.2/A10"/>
<pin name="P2.3/A11"/>
<pin name="P2.4/A12"/>
<pin name="P2.5/A13"/>
<pin name="P2.6/A14"/>
<pin name="P2.7/A15"/>
<pin name="P4.4" direction="in"/>
<pin name="P4.5" direction="in"/>
<pin name="P4.6" direction="in"/>
<pin name="P4.7" direction="in"/>
<pin name="AREFP" direction="in"/>
<pin name="!TST" direction="in"/>
</symbol>
<symbol name="P-AT89C51SND1C">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="PVSS" direction="pwr"/>
<pin name="UVDD" direction="pwr"/>
<pin name="UVSS" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
</symbol>
<symbol name="AT89C51">
<pin name="!EA!/VPP" direction="in"/>
<pin name="P0.0_AD0"/>
<pin name="P0.1_AD1"/>
<pin name="P0.2_AD2"/>
<pin name="P0.3_AD3"/>
<pin name="P0.4_AD4"/>
<pin name="P0.5_AD5"/>
<pin name="P0.6_AD6"/>
<pin name="P0.7_AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE/!PROG" direction="out"/>
<pin name="!PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AT89S51">
<pin name="!EA!/VPP" direction="in"/>
<pin name="P0.0_AD0"/>
<pin name="P0.1_AD1"/>
<pin name="P0.2_AD2"/>
<pin name="P0.3_AD3"/>
<pin name="P0.4_AD4"/>
<pin name="P0.5_AD5"/>
<pin name="P0.6_AD6"/>
<pin name="P0.7_AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE/!PROG" direction="out"/>
<pin name="!PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5_MOSI"/>
<pin name="P1.6_MISO"/>
<pin name="P1.7_SCK"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="T89C51CC02">
<pin name="P4.0/RXDC"/>
<pin name="P4.1/TXDC"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="P2.0"/>
<pin name="P2.1"/>
<pin name="P1.0/AN0/T2"/>
<pin name="P1.1/AN1/T2EX"/>
<pin name="P1.2/AN2/ECI"/>
<pin name="P1.3/AN3/CEX0"/>
<pin name="P1.4/AN4/CEX1"/>
<pin name="P1.5/AN5"/>
<pin name="P1.6/AN6"/>
<pin name="P1.7/AN7"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6"/>
<pin name="P3.7"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VAREF" direction="in"/>
<pin name="VAGND" direction="in"/>
<pin name="VAVCC" direction="in"/>
</symbol>
<symbol name="T89C51CC02-SO24">
<pin name="P4.0/RXDC"/>
<pin name="P4.1/TXDC"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="P1.0/AN0/T2"/>
<pin name="P1.1/AN1/T2EX"/>
<pin name="P1.2/AN2/ECI"/>
<pin name="P1.3/AN3/CEX0"/>
<pin name="P1.4/AN4/CEX1"/>
<pin name="P1.5/AN5"/>
<pin name="P1.6/AN6"/>
<pin name="P1.7/AN7"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VAREF" direction="in"/>
<pin name="VAGND" direction="in"/>
<pin name="VAVCC" direction="in"/>
</symbol>
<symbol name="AT91RM9200_BGA">
<pin name="ICETCK" direction="in"/>
<pin name="ICETDI" direction="in"/>
<pin name="ICETMS" direction="in"/>
<pin name="JTAGSEL" direction="in"/>
<pin name="NTRST" direction="in"/>
<pin name="TST0" direction="in"/>
<pin name="TST1" direction="in"/>
<pin name="D_0"/>
<pin name="D_1"/>
<pin name="D_10"/>
<pin name="D_11"/>
<pin name="D_12"/>
<pin name="D_13"/>
<pin name="D_14"/>
<pin name="D_15"/>
<pin name="D_2"/>
<pin name="D_3"/>
<pin name="D_4"/>
<pin name="D_5"/>
<pin name="D_6"/>
<pin name="D_7"/>
<pin name="D_8"/>
<pin name="D_9"/>
<pin name="NRW0NWE"/>
<pin name="NRW1_NUB_DQM1"/>
<pin name="PA0"/>
<pin name="PA1"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="PA16"/>
<pin name="PA17"/>
<pin name="PA18"/>
<pin name="PA19"/>
<pin name="PA2"/>
<pin name="PA20"/>
<pin name="PA21"/>
<pin name="PA22"/>
<pin name="PA23"/>
<pin name="PA24"/>
<pin name="PA25"/>
<pin name="PA26"/>
<pin name="PA27"/>
<pin name="PA28"/>
<pin name="PA29"/>
<pin name="PA3"/>
<pin name="PA30"/>
<pin name="PA31"/>
<pin name="PA4"/>
<pin name="PA5"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA8"/>
<pin name="PA9"/>
<pin name="PB0"/>
<pin name="PB1"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PB16"/>
<pin name="PB17"/>
<pin name="PB18"/>
<pin name="PB19"/>
<pin name="PB2"/>
<pin name="PB20"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB24"/>
<pin name="PB25"/>
<pin name="PB26"/>
<pin name="PB27"/>
<pin name="PB28"/>
<pin name="PB29"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB9"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC10"/>
<pin name="PC11"/>
<pin name="PC12"/>
<pin name="PC13"/>
<pin name="PC14"/>
<pin name="PC15"/>
<pin name="PC16"/>
<pin name="PC17"/>
<pin name="PC18"/>
<pin name="PC19"/>
<pin name="PC2"/>
<pin name="PC20"/>
<pin name="PC21"/>
<pin name="PC22"/>
<pin name="PC23"/>
<pin name="PC24"/>
<pin name="PC25"/>
<pin name="PC26"/>
<pin name="PC27"/>
<pin name="PC28"/>
<pin name="PC29"/>
<pin name="PC3"/>
<pin name="PC30"/>
<pin name="PC31"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PC8"/>
<pin name="PC9"/>
<pin name="PD0"/>
<pin name="PD1"/>
<pin name="PD10"/>
<pin name="PD11"/>
<pin name="PD12"/>
<pin name="PD13"/>
<pin name="PD14"/>
<pin name="PD15"/>
<pin name="PD16"/>
<pin name="PD17"/>
<pin name="PD18"/>
<pin name="PD19"/>
<pin name="PD2"/>
<pin name="PD20"/>
<pin name="PD21"/>
<pin name="PD22"/>
<pin name="PD23"/>
<pin name="PD24"/>
<pin name="PD25"/>
<pin name="PD26"/>
<pin name="PD27"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PD8"/>
<pin name="PD9"/>
<pin name="A_10" direction="out"/>
<pin name="A10_SDRAM" direction="out"/>
<pin name="A_11" direction="out"/>
<pin name="A_12" direction="out"/>
<pin name="A_13" direction="out"/>
<pin name="A_14" direction="out"/>
<pin name="A_15" direction="out"/>
<pin name="A16_BA0" direction="out"/>
<pin name="A17_BA1" direction="out"/>
<pin name="A_18" direction="out"/>
<pin name="A_19" direction="out"/>
<pin name="A1_DQM2" direction="out"/>
<pin name="A_2" direction="out"/>
<pin name="A_20" direction="out"/>
<pin name="A_21" direction="out"/>
<pin name="A_22" direction="out"/>
<pin name="A_3" direction="out"/>
<pin name="A_4" direction="out"/>
<pin name="A_5" direction="out"/>
<pin name="A_6" direction="out"/>
<pin name="A_7" direction="out"/>
<pin name="A_8" direction="out"/>
<pin name="A_9" direction="out"/>
<pin name="CAS" direction="out"/>
<pin name="ICETDO" direction="out"/>
<pin name="NBS3" direction="out"/>
<pin name="NCS0_BFCS" direction="out"/>
<pin name="NCS1_SDCS" direction="out"/>
<pin name="NCS2" direction="out"/>
<pin name="NCS3" direction="out"/>
<pin name="NLBA0_DQM0" direction="out"/>
<pin name="NRDNOE" direction="out"/>
<pin name="RAS" direction="out"/>
<pin name="SDRAMCKE" direction="out"/>
<pin name="WE" direction="out"/>
<pin name="DM" direction="pwr"/>
<pin name="DP" direction="pwr"/>
<pin name="HDMA" direction="pwr"/>
<pin name="HDMB" direction="pwr"/>
<pin name="HDPA" direction="pwr"/>
<pin name="HDPB" direction="pwr"/>
<pin name="NRST" direction="pwr"/>
<pin name="OSC32K_XIN" direction="pwr"/>
<pin name="OSC32K_XOUT" direction="pwr"/>
<pin name="OSC9M_XIN" direction="pwr"/>
<pin name="OSC9M_XOUT" direction="pwr"/>
<pin name="PLL_A_RC" direction="pwr"/>
<pin name="PLL_B_RC" direction="pwr"/>
<pin name="SDRAMCLK" direction="pwr"/>
<pin name="MIX33VDD@1" direction="pwr"/>
<pin name="MIX33VDD@2" direction="pwr"/>
<pin name="MIX33VDD@3" direction="pwr"/>
<pin name="MIX33VDD@4" direction="pwr"/>
<pin name="MIX33VDD@5" direction="pwr"/>
<pin name="MIX33VDD@6" direction="pwr"/>
<pin name="MIX33VDD@7" direction="pwr"/>
<pin name="MIX33VDD@8" direction="pwr"/>
<pin name="MIX33VDD@9" direction="pwr"/>
<pin name="MIX33VDD@10" direction="pwr"/>
<pin name="MIX33VDD@11" direction="pwr"/>
<pin name="MIX33VDD@12" direction="pwr"/>
<pin name="MIX33VDD@13" direction="pwr"/>
<pin name="MIX33VDD@14" direction="pwr"/>
<pin name="MIX33VDD@15" direction="pwr"/>
<pin name="MIX33VDD@16" direction="pwr"/>
<pin name="MIX33VDD@17" direction="pwr"/>
<pin name="MIX33VDD@18" direction="pwr"/>
<pin name="MIX33VDD@19" direction="pwr"/>
<pin name="MIX33VDD@20" direction="pwr"/>
<pin name="MIX33VDD@21" direction="pwr"/>
<pin name="MIX33VSS@1" direction="pwr"/>
<pin name="MIX33VSS@2" direction="pwr"/>
<pin name="MIX33VSS@3" direction="pwr"/>
<pin name="MIX33VSS@4" direction="pwr"/>
<pin name="MIX33VSS@5" direction="pwr"/>
<pin name="MIX33VSS@6" direction="pwr"/>
<pin name="MIX33VSS@7" direction="pwr"/>
<pin name="MIX33VSS@8" direction="pwr"/>
<pin name="MIX33VSS@9" direction="pwr"/>
<pin name="MIX33VSS@10" direction="pwr"/>
<pin name="MIX33VSS@11" direction="pwr"/>
<pin name="MIX33VSS@12" direction="pwr"/>
<pin name="MIX33VSS@13" direction="pwr"/>
<pin name="MIX33VSS@14" direction="pwr"/>
<pin name="MIX33VSS@15" direction="pwr"/>
<pin name="MIX33VSS@16" direction="pwr"/>
<pin name="MIX33VSS@17" direction="pwr"/>
<pin name="MIX33VSS@18" direction="pwr"/>
<pin name="MIX33VSS@19" direction="pwr"/>
<pin name="MIX33VSS@20" direction="pwr"/>
<pin name="MIX33VSS@21" direction="pwr"/>
<pin name="VDDI@1" direction="pwr"/>
<pin name="VDDI@2" direction="pwr"/>
<pin name="VDDI@3" direction="pwr"/>
<pin name="VDDI@4" direction="pwr"/>
<pin name="VDDI@5" direction="pwr"/>
<pin name="VDDI@6" direction="pwr"/>
<pin name="VDDI@7" direction="pwr"/>
<pin name="VDDI@8" direction="pwr"/>
<pin name="VDDI@9" direction="pwr"/>
<pin name="VSSI@1" direction="pwr"/>
<pin name="VSSI@2" direction="pwr"/>
<pin name="VSSI@3" direction="pwr"/>
<pin name="VSSI@4" direction="pwr"/>
<pin name="VSSI@5" direction="pwr"/>
<pin name="VSSI@6" direction="pwr"/>
<pin name="VSSI@7" direction="pwr"/>
<pin name="VSSI@8" direction="pwr"/>
<pin name="VSSI@9" direction="pwr"/>
</symbol>
<symbol name="ATF16V8B">
<pin name="CLK" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="I2" direction="in"/>
<pin name="I3" direction="in"/>
<pin name="I4" direction="in"/>
<pin name="I5" direction="in"/>
<pin name="I6" direction="in"/>
<pin name="I7" direction="in"/>
<pin name="I8" direction="in"/>
<pin name="O1" direction="out"/>
<pin name="O2" direction="out"/>
<pin name="O3" direction="out"/>
<pin name="O4" direction="out"/>
<pin name="O5" direction="out"/>
<pin name="O6" direction="out"/>
<pin name="O7" direction="out"/>
<pin name="O8" direction="out"/>
<pin name="OE" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="23-I/O">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="23-I/O-2">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
</symbol>
<symbol name="32-I/O-M16-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M16-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-M32-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M32-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="MEGA64">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="MEGA128">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
</symbol>
<symbol name="MEGA169">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PCINT0)PE0"/>
<pin name="(TXD/PCINT1)PE1"/>
<pin name="(XCK0/AIN0/PCINT2)PE2"/>
<pin name="(AIN1/PCINT3)PE3"/>
<pin name="(USCK/SCL/PCINT4)PE4"/>
<pin name="(DI/SDA/PCINT5)PE5"/>
<pin name="(DO/PCINT6)PE6"/>
<pin name="(CLKO/PCINT7)PE7"/>
<pin name="(SEG15)PD7"/>
<pin name="(SEG16)PD6"/>
<pin name="(SEG17)PD5"/>
<pin name="(SEG18)PD4"/>
<pin name="(SEG19)PD3"/>
<pin name="(SEG20)PD2"/>
<pin name="(SEG21/INT0)PD1"/>
<pin name="(SEG22/ICP)PD0"/>
<pin name="(SEG5)PC7" direction="out"/>
<pin name="(SEG6)PC6" direction="out"/>
<pin name="(SEG7)PC5" direction="out"/>
<pin name="(SEG8)PC4" direction="out"/>
<pin name="(SEG9)PC3" direction="out"/>
<pin name="(SEG10)PC2" direction="out"/>
<pin name="(SEG11)PC1" direction="out"/>
<pin name="(SEG12)PC0" direction="out"/>
<pin name="(OC2A/PCINT15)PB7"/>
<pin name="(OC1B/PCINT14)PB6"/>
<pin name="(OC1A/PCINT13)PB5"/>
<pin name="(OC0A/PCINT12)PB4"/>
<pin name="(MISO/PCINT11)PB3"/>
<pin name="(MOSI/PCINT10)PB2"/>
<pin name="(SCK/PCINT9)PB1"/>
<pin name="(SS/PCINT8)PB0"/>
<pin name="(SEG2)PA6"/>
<pin name="(SEG3)PA7"/>
<pin name="(SEG1)PA5"/>
<pin name="(SEG0)PA4"/>
<pin name="(COM3)PA3"/>
<pin name="(COM2)PA2"/>
<pin name="(COM1)PA1"/>
<pin name="(COM0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1(TOSC1)"/>
<pin name="XTAL2(TOSC2)"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(T1/SEG24)"/>
<pin name="PG4(T0/SEG23)"/>
<pin name="PG0(SEG14)"/>
<pin name="PG1(SEG13)"/>
<pin name="PG2(SEG4)"/>
<pin name="PG5(RESET)" direction="in" function="dot"/>
<pin name="LCDCAP" direction="in"/>
</symbol>
<symbol name="MEGA323-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MEGA323">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="32-I/O-M8515-A">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(XCK)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="32-I/O-7">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(XCK)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
</symbol>
<symbol name="32-I/O-M8535-A">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="32-I/O-M8535-P">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/INT2)PB3"/>
<pin name="(AIN0/OC0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="(SDA)PC1"/>
<pin name="(SCL)PC0"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
</symbol>
<symbol name="AT89C5131">
<pin name="!EA!/VPP" direction="in"/>
<pin name="P0.0_AD0"/>
<pin name="P0.1_AD1"/>
<pin name="P0.2_AD2"/>
<pin name="P0.3_AD3"/>
<pin name="P0.4_AD4"/>
<pin name="P0.5_AD5"/>
<pin name="P0.6_AD6"/>
<pin name="P0.7_AD7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="ALE"/>
<pin name="!PSEN" direction="out"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0/T2/KIN0"/>
<pin name="P1.1/T2EX/KIN1/SS"/>
<pin name="P1.2/ECI/KIN2"/>
<pin name="P1.3/CEX0/KIN3"/>
<pin name="P1.4/CEX1/KIN4"/>
<pin name="P1.5/CEX2/KIN5/MISO"/>
<pin name="P1.6/CEX3/KIN6/SCK"/>
<pin name="P1.7/CEX4/KIN7/MOSI"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="PLLF"/>
<pin name="FREV"/>
<pin name="P4.0/SCL"/>
<pin name="P4.1/SDA"/>
<pin name="AVSS" direction="pwr"/>
</symbol>
<symbol name="AT89C5132">
<pin name="VDD@1" direction="pwr"/>
<pin name="P0.0_AD0"/>
<pin name="P0.1_AD1"/>
<pin name="P0.2_AD2"/>
<pin name="P0.3_AD3"/>
<pin name="P0.4_AD4"/>
<pin name="P0.5_AD5"/>
<pin name="P0.6_AD6"/>
<pin name="P0.7_AD7"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="ALE"/>
<pin name="P4.3/!SS"/>
<pin name="P2.0_A8"/>
<pin name="P2.1_A9"/>
<pin name="P2.2_A10"/>
<pin name="P2.3_A11"/>
<pin name="P2.4_A12"/>
<pin name="P2.5_A13"/>
<pin name="P2.6_A14"/>
<pin name="P2.7_A15"/>
<pin name="P1.0/KIN0"/>
<pin name="P1.1/KIN1"/>
<pin name="P1.2/KIN2"/>
<pin name="P1.3/KIN3"/>
<pin name="P1.6/SCL"/>
<pin name="P1.7/SDA"/>
<pin name="P3.0/RXD"/>
<pin name="P3.1/TXD"/>
<pin name="P3.2/!INT0"/>
<pin name="P3.3/!INT1"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/!WR"/>
<pin name="P3.7/!RD"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="P4.0/MISO"/>
<pin name="P4.1/MOSI"/>
<pin name="P4.2/SCK"/>
<pin name="P4.4"/>
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="FILT" direction="in"/>
<pin name="DCLK" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="DSEL" direction="out"/>
<pin name="SCLK" direction="out"/>
<pin name="MCLK" direction="out"/>
<pin name="MCMD"/>
<pin name="MDAT"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AREFP" direction="in"/>
<pin name="AREFN" direction="in"/>
<pin name="!ISP"/>
<pin name="!TST" direction="in"/>
<pin name="UVDD" direction="pwr"/>
<pin name="UVSS" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="PVSS" direction="pwr"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
</symbol>
<symbol name="23-I/O_MI">
<pin name="PB5(SCK)"/>
<pin name="PB7(XTAL2/TOSC2)"/>
<pin name="PB6(XTAL1/TOSC1)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="AVCC" direction="pwr"/>
<pin name="PB4(MISO)"/>
<pin name="PB3(MOSI/OC2)"/>
<pin name="PB2(SS/OC1B)"/>
<pin name="PB1(OC1A)"/>
<pin name="PB0(ICP)"/>
<pin name="PD7(AIN1)"/>
<pin name="PD6(AIN0)"/>
<pin name="PD5(T1)"/>
<pin name="PD4(XCK/T0)"/>
<pin name="PD3(INT1)"/>
<pin name="PD2(INT0)"/>
<pin name="PD1(TXD)"/>
<pin name="PD0(RXD)"/>
<pin name="ADC7"/>
<pin name="ADC6"/>
<pin name="PC5(ADC5/SCL)"/>
<pin name="PC4(ADC4/SDA)"/>
<pin name="PC3(ADC3)"/>
<pin name="PC2(ADC2)"/>
<pin name="PC1(ADC1)"/>
<pin name="PC0(ADC0)"/>
<pin name="PC6(/RESET)" function="dot"/>
<pin name="THERMAL" direction="pas"/>
</symbol>
<symbol name="32-I/O-M16-A_M">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="32-I/O-M32-A_M">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="(TDI)PC5"/>
<pin name="(TDO)PC4"/>
<pin name="(TMS)PC3"/>
<pin name="(TCK)PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="MEGA64-M">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="MEGA128-M">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PDI)PE0"/>
<pin name="(TXD/PDO)PE1"/>
<pin name="(XCK0/AIN0)PE2"/>
<pin name="(OC3A/AIN1)PE3"/>
<pin name="(OC3B/INT4)PE4"/>
<pin name="(OC3C/INT5)PE5"/>
<pin name="(T3/INT6)PE6"/>
<pin name="(IC3/INT7)PE7"/>
<pin name="(T2)PD7"/>
<pin name="(T1)PD6"/>
<pin name="(XCK1)PD5"/>
<pin name="(IC1)PD4"/>
<pin name="(TXD1/INT3)PD3"/>
<pin name="(RXD1/INT2)PD2"/>
<pin name="(SDA/INT1)PD1"/>
<pin name="(SCL/INT0)PD0"/>
<pin name="(A15)PC7" direction="out"/>
<pin name="(A14)PC6" direction="out"/>
<pin name="(A13)PC5" direction="out"/>
<pin name="(A12)PC4" direction="out"/>
<pin name="(A11)PC3" direction="out"/>
<pin name="(A10)PC2" direction="out"/>
<pin name="(A9)PC1" direction="out"/>
<pin name="(A8)PC0" direction="out"/>
<pin name="(OC2/OC1C)PB7"/>
<pin name="(OC1B)PB6"/>
<pin name="(OC1A)PB5"/>
<pin name="(OC0)PB4"/>
<pin name="(MISO)PB3"/>
<pin name="(MOSI)PB2"/>
<pin name="(SCK)PB1"/>
<pin name="(SS)PB0"/>
<pin name="(AD6)PA6"/>
<pin name="(AD7)PA7"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(TOSC2)"/>
<pin name="PG4(TOSC1)"/>
<pin name="PG0(WR)" function="dot"/>
<pin name="PG1(RD)" function="dot"/>
<pin name="PG2(ALE)"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="PEN" direction="in" function="dot"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="MEGA169-M">
<pin name="PF0(ADC0)" direction="in"/>
<pin name="PF1(ADC1)" direction="in"/>
<pin name="PF2(ADC2)" direction="in"/>
<pin name="PF3(ADC3)" direction="in"/>
<pin name="PF4(ADC4/TCK)" direction="in"/>
<pin name="PF5(ADC5/TMS)" direction="in"/>
<pin name="PF6(ADC6/TDO)" direction="in"/>
<pin name="PF7(ADC7/TDI)" direction="in"/>
<pin name="(RXD/PCINT0)PE0"/>
<pin name="(TXD/PCINT1)PE1"/>
<pin name="(XCK0/AIN0/PCINT2)PE2"/>
<pin name="(AIN1/PCINT3)PE3"/>
<pin name="(USCK/SCL/PCINT4)PE4"/>
<pin name="(DI/SDA/PCINT5)PE5"/>
<pin name="(DO/PCINT6)PE6"/>
<pin name="(CLKO/PCINT7)PE7"/>
<pin name="(SEG15)PD7"/>
<pin name="(SEG16)PD6"/>
<pin name="(SEG17)PD5"/>
<pin name="(SEG18)PD4"/>
<pin name="(SEG19)PD3"/>
<pin name="(SEG20)PD2"/>
<pin name="(SEG21/INT0)PD1"/>
<pin name="(SEG22/ICP)PD0"/>
<pin name="(SEG5)PC7" direction="out"/>
<pin name="(SEG6)PC6" direction="out"/>
<pin name="(SEG7)PC5" direction="out"/>
<pin name="(SEG8)PC4" direction="out"/>
<pin name="(SEG9)PC3" direction="out"/>
<pin name="(SEG10)PC2" direction="out"/>
<pin name="(SEG11)PC1" direction="out"/>
<pin name="(SEG12)PC0" direction="out"/>
<pin name="(OC2A/PCINT15)PB7"/>
<pin name="(OC1B/PCINT14)PB6"/>
<pin name="(OC1A/PCINT13)PB5"/>
<pin name="(OC0A/PCINT12)PB4"/>
<pin name="(MISO/PCINT11)PB3"/>
<pin name="(MOSI/PCINT10)PB2"/>
<pin name="(SCK/PCINT9)PB1"/>
<pin name="(SS/PCINT8)PB0"/>
<pin name="(SEG2)PA6"/>
<pin name="(SEG3)PA7"/>
<pin name="(SEG1)PA5"/>
<pin name="(SEG0)PA4"/>
<pin name="(COM3)PA3"/>
<pin name="(COM2)PA2"/>
<pin name="(COM1)PA1"/>
<pin name="(COM0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1(TOSC1)"/>
<pin name="XTAL2(TOSC2)"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PG3(T1/SEG24)"/>
<pin name="PG4(T0/SEG23)"/>
<pin name="PG0(SEG14)"/>
<pin name="PG1(SEG13)"/>
<pin name="PG2(SEG4)"/>
<pin name="PG5(RESET)" direction="in" function="dot"/>
<pin name="LCDCAP" direction="in"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="32-I/O-M8515-A_M">
<pin name="(AD7)PA7"/>
<pin name="(AD6)PA6"/>
<pin name="(AD5)PA5"/>
<pin name="(AD4)PA4"/>
<pin name="(AD3)PA3"/>
<pin name="(AD2)PA2"/>
<pin name="(AD1)PA1"/>
<pin name="(AD0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1)PB3"/>
<pin name="(AIN0)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/OC0)PB0"/>
<pin name="(A15)PC7"/>
<pin name="(A14)PC6"/>
<pin name="(A13)PC5"/>
<pin name="(A12)PC4"/>
<pin name="(A11)PC3"/>
<pin name="(A10)PC2"/>
<pin name="(A9)PC1"/>
<pin name="(A8)PC0"/>
<pin name="PE2(OC1B)"/>
<pin name="PE1(ALE)"/>
<pin name="PE0(ICP/INT2)"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(XCK)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(WR)PD6"/>
<pin name="(RD)PD7"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="32-I/O-M8535-A_M">
<pin name="(ADC7)PA7"/>
<pin name="(ADC6)PA6"/>
<pin name="(ADC5)PA5"/>
<pin name="(ADC4)PA4"/>
<pin name="(ADC3)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="(SCK)PB7"/>
<pin name="(MISO)PB6"/>
<pin name="(MOSI)PB5"/>
<pin name="(SS)PB4"/>
<pin name="(AIN1/OC0)PB3"/>
<pin name="(AIN0/INT2)PB2"/>
<pin name="(T1)PB1"/>
<pin name="(T0/XCK)PB0"/>
<pin name="(TOSC2)PC7"/>
<pin name="(TOSC1)PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1(SDA)"/>
<pin name="PC0(SCL)"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="(RXD)PD0"/>
<pin name="(TXD)PD1"/>
<pin name="(INT0)PD2"/>
<pin name="(INT1)PD3"/>
<pin name="(OC1B)PD4"/>
<pin name="(OC1A)PD5"/>
<pin name="(ICP)PD6"/>
<pin name="(OC2)PD7"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="TINY26_M">
<pin name="(ADC8/XTAL2)PB5"/>
<pin name="(ADC7/XTAL1)PB4"/>
<pin name="(OC1B)PB3"/>
<pin name="(SCK/SCL/!OC1B!)PB2"/>
<pin name="(MISO/DO/OC1A)PB1"/>
<pin name="(MOSI/DI/SDA/!OC1A!)PB0"/>
<pin name="(ADC6/AIN1)PA7"/>
<pin name="(ADC5/AIN0)PA6"/>
<pin name="(ADC4)PA5"/>
<pin name="(ADC3)PA4"/>
<pin name="(AREF)PA3"/>
<pin name="(ADC2)PA2"/>
<pin name="(ADC1)PA1"/>
<pin name="(ADC0)PA0"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="(ADC10/!RESET!)PB7"/>
<pin name="(ADC9/INT0/T0)PB6"/>
<pin name="GND@1" direction="pwr"/>
<pin name="THERMAL" direction="in"/>
</symbol>
<symbol name="ATMEGA644">
<pin name="(PCINT31/OC2A)PD7"/>
<pin name="(PCINT30/OC2B/ICP)PD6"/>
<pin name="(PCINT29/OC1A)PD5"/>
<pin name="(PCINT28/OC1B)PD4"/>
<pin name="(PCINT27/INT1)PD3"/>
<pin name="(PCINT26/INT0)PD2"/>
<pin name="(PCINT25/TXD0)PD1"/>
<pin name="(PCINT24/RXD0)PD0"/>
<pin name="(PCINT23/TOSC2)PC7" direction="out"/>
<pin name="(PCINT22/TOSC1)PC6" direction="out"/>
<pin name="(PCINT21/TDI)PC5" direction="out"/>
<pin name="(PCINT20/TDO)PC4" direction="out"/>
<pin name="(PCINT19/TMS)PC3" direction="out"/>
<pin name="(PCINT18/TCK)PC2" direction="out"/>
<pin name="(PCINT17/SDA)PC1" direction="out"/>
<pin name="(PCINT16/SCL)PC0" direction="out"/>
<pin name="(PCINT15/SCK)PB7"/>
<pin name="(PCINT14/MISO)PB6"/>
<pin name="(PCINT13/MOSI)PB5"/>
<pin name="(PCINT12/OC0B/!SS!)PB4"/>
<pin name="(PCINT11/OC0A/AIN1)PB3"/>
<pin name="(PCINT10/INT2/AIN0)PB2"/>
<pin name="(PCINT9/CLKO/T1)PB1"/>
<pin name="(PCINT8/XCK0/T0)PB0"/>
<pin name="(PCINT6/ADC6)PA6"/>
<pin name="(PCINT7/ADC7)PA7"/>
<pin name="(PCINT5/ADC5)PA5"/>
<pin name="(PCINT4/ADC4)PA4"/>
<pin name="(PCINT3/ADC3)PA3"/>
<pin name="(PCINT2/ADC2)PA2"/>
<pin name="(PCINT1/ADC1)PA1"/>
<pin name="(PCINT0/ADC0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="ATMEGA644E">
<pin name="(PCINT31/OC2A)PD7"/>
<pin name="(PCINT30/OC2B/ICP)PD6"/>
<pin name="(PCINT29/OC1A)PD5"/>
<pin name="(PCINT28/OC1B)PD4"/>
<pin name="(PCINT27/INT1)PD3"/>
<pin name="(PCINT26/INT0)PD2"/>
<pin name="(PCINT25/TXD0)PD1"/>
<pin name="(PCINT24/RXD0)PD0"/>
<pin name="(PCINT23/TOSC2)PC7" direction="out"/>
<pin name="(PCINT22/TOSC1)PC6" direction="out"/>
<pin name="(PCINT21/TDI)PC5" direction="out"/>
<pin name="(PCINT20/TDO)PC4" direction="out"/>
<pin name="(PCINT19/TMS)PC3" direction="out"/>
<pin name="(PCINT18/TCK)PC2" direction="out"/>
<pin name="(PCINT17/SDA)PC1" direction="out"/>
<pin name="(PCINT16/SCL)PC0" direction="out"/>
<pin name="(PCINT15/SCK)PB7"/>
<pin name="(PCINT14/MISO)PB6"/>
<pin name="(PCINT13/MOSI)PB5"/>
<pin name="(PCINT12/OC0B/!SS!)PB4"/>
<pin name="(PCINT11/OC0A/AIN1)PB3"/>
<pin name="(PCINT10/INT2/AIN0)PB2"/>
<pin name="(PCINT9/CLKO/T1)PB1"/>
<pin name="(PCINT8/XCK0/T0)PB0"/>
<pin name="(PCINT6/ADC6)PA6"/>
<pin name="(PCINT7/ADC7)PA7"/>
<pin name="(PCINT5/ADC5)PA5"/>
<pin name="(PCINT4/ADC4)PA4"/>
<pin name="(PCINT3/ADC3)PA3"/>
<pin name="(PCINT2/ADC2)PA2"/>
<pin name="(PCINT1/ADC1)PA1"/>
<pin name="(PCINT0/ADC0)PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="in" function="dot"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="EXP" direction="pwr"/>
</symbol>
<symbol name="AT91SAM7X">
<pin name="ADVREF"/>
<pin name="GND@1"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="VDDOUT@1"/>
<pin name="VDDIN@1"/>
<pin name="PB27/AD0"/>
<pin name="PB28/AD1"/>
<pin name="PB29/AD2"/>
<pin name="PB30/AD3"/>
<pin name="PA8/PGMM0"/>
<pin name="PA9/PGMM1"/>
<pin name="VDDCORE@1"/>
<pin name="GND@2"/>
<pin name="VDDIO@1"/>
<pin name="PA10/PGMM2"/>
<pin name="PA11/PGMM3"/>
<pin name="PA12/PGMD0"/>
<pin name="PA13/PGMD1"/>
<pin name="PA14/PGMD2"/>
<pin name="PA15/PGMD3"/>
<pin name="PA16/PGMD4"/>
<pin name="PA17/PGMD5"/>
<pin name="PA18/PGMD6"/>
<pin name="PB9"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PB16"/>
<pin name="PB17"/>
<pin name="PB18"/>
<pin name="PA19/PGMD7"/>
<pin name="PA20/PGMD8"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB24"/>
<pin name="PB25"/>
<pin name="PB26"/>
<pin name="GND@3"/>
<pin name="VDDIO@2"/>
<pin name="VDDCORE@2"/>
<pin name="PB0"/>
<pin name="VDDIO@3"/>
<pin name="PA21/PGMD9"/>
<pin name="PA22/PGMD10"/>
<pin name="TDI"/>
<pin name="GND@4"/>
<pin name="PA23/PGMD11"/>
<pin name="PA24/PGMD12"/>
<pin name="NRST"/>
<pin name="TST"/>
<pin name="PA25/PGMD13"/>
<pin name="PA26/PGMD14"/>
<pin name="VDDIO@4"/>
<pin name="VDDCORE@3"/>
<pin name="PB19"/>
<pin name="PB20"/>
<pin name="GND@5"/>
<pin name="PA27/PGMD15"/>
<pin name="PA28"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4/PGMNCMD"/>
<pin name="PA5/PGMRDY"/>
<pin name="PA6/PGMNOE"/>
<pin name="PA7/PGMNVALID"/>
<pin name="PA29"/>
<pin name="TDO"/>
<pin name="JTAGSEL"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="PA30"/>
<pin name="PA0/PGMEN0"/>
<pin name="PA1/PGMEN1"/>
<pin name="GND@6"/>
<pin name="VDDIO@5"/>
<pin name="VDDCORE@4"/>
<pin name="ERASE"/>
<pin name="DDM"/>
<pin name="DDP"/>
<pin name="VDDFLASH"/>
<pin name="GND@7"/>
<pin name="XOUT"/>
<pin name="PLLRC"/>
<pin name="VDDPLL"/>
<pin name="XIN/PGMCK"/>
</symbol>
<symbol name="AT91SAM7X-BGA">
<pin name="ADVREF"/>
<pin name="GND@1"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="VDDOUT@1" direction="out"/>
<pin name="VDDIN@1"/>
<pin name="PB27/AD0"/>
<pin name="PB28/AD1"/>
<pin name="PB29/AD2"/>
<pin name="PB30/AD3"/>
<pin name="PA8/PGMM0"/>
<pin name="PA9/PGMM1"/>
<pin name="VDDCORE@1"/>
<pin name="GND@2"/>
<pin name="VDDIO@1"/>
<pin name="PA10/PGMM2"/>
<pin name="PA11/PGMM3"/>
<pin name="PA12/PGMD0"/>
<pin name="PA13/PGMD1"/>
<pin name="PA14/PGMD2"/>
<pin name="PA15/PGMD3"/>
<pin name="PA16/PGMD4"/>
<pin name="PA17/PGMD5"/>
<pin name="PA18/PGMD6"/>
<pin name="PB9"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
<pin name="PB8"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PB16"/>
<pin name="PB17"/>
<pin name="PB18"/>
<pin name="PA19/PGMD7"/>
<pin name="PA20/PGMD8"/>
<pin name="PB21"/>
<pin name="PB22"/>
<pin name="PB23"/>
<pin name="PB24"/>
<pin name="PB25"/>
<pin name="PB26"/>
<pin name="GND@3"/>
<pin name="VDDIO@2"/>
<pin name="VDDCORE@2"/>
<pin name="PB0"/>
<pin name="VDDIO@3"/>
<pin name="PA21/PGMD9"/>
<pin name="PA22/PGMD10"/>
<pin name="TDI"/>
<pin name="GND@4"/>
<pin name="PA23/PGMD11"/>
<pin name="PA24/PGMD12"/>
<pin name="NRST"/>
<pin name="TST"/>
<pin name="PA25/PGMD13"/>
<pin name="PA26/PGMD14"/>
<pin name="VDDIO@4"/>
<pin name="VDDCORE@3"/>
<pin name="PB19"/>
<pin name="PB20"/>
<pin name="GND@5"/>
<pin name="PA27/PGMD15"/>
<pin name="PA28"/>
<pin name="PA2"/>
<pin name="PA3"/>
<pin name="PA4/PGMNCMD"/>
<pin name="PA5/PGMRDY"/>
<pin name="PA6/PGMNOE"/>
<pin name="PA7/PGMNVALID"/>
<pin name="PA29"/>
<pin name="TDO"/>
<pin name="JTAGSEL"/>
<pin name="TMS"/>
<pin name="TCK"/>
<pin name="PA30"/>
<pin name="PA0/PGMEN0"/>
<pin name="PA1/PGMEN1"/>
<pin name="GND@6"/>
<pin name="VDDCORE@5"/>
<pin name="VDDCORE@4"/>
<pin name="ERASE"/>
<pin name="DDM"/>
<pin name="DDP"/>
<pin name="VDDFLASH"/>
<pin name="GND@7"/>
<pin name="XOUT" direction="out"/>
<pin name="PLLRC"/>
<pin name="VDDPLL"/>
<pin name="XIN/PGMCK"/>
</symbol>
<symbol name="AT93C46A">
<pin name="DO" direction="out"/>
<pin name="DI" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="SK" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="DC" direction="nc"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TINY13">
<pin name="PB5/PCINT5/!RESET!/ADC0/DW"/>
<pin name="PB3/PCINT3/CLKI/ADC3"/>
<pin name="PB4/PCINT4/ADC2"/>
<pin name="PB0/PCINT0/AIN0/OC0A/MOSI"/>
<pin name="PB1/PCINT1/AIN1/OC0B/INT0/MISO"/>
<pin name="PB2/PCINT2/SCK/ADC1/T0"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="T7024">
<pin name="RX_ON" direction="in"/>
<pin name="PU" direction="in"/>
<pin name="VS_LNA" direction="in"/>
<pin name="LNA_OUT" direction="in"/>
<pin name="LNA_IN" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="PA_IN" direction="in"/>
<pin name="V3_PA_OUT@1" direction="pas"/>
<pin name="V1_PA" direction="pas"/>
<pin name="V2_PA@1" direction="pas"/>
<pin name="R_SWITCH" direction="in"/>
<pin name="SWITCH_OUT" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="V3_PA_OUT@2" direction="pas"/>
<pin name="V3_PA_OUT@3" direction="pas"/>
<pin name="V2_PA@2" direction="pas"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="XMEGA16A4">
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="PC7"/>
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="PB3"/>
<pin name="PB2"/>
<pin name="PB1"/>
<pin name="PB0"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="PR0(XT2)"/>
<pin name="PR1(XT1)"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PDI_DATA"/>
<pin name="GND2" direction="pwr"/>
<pin name="!RESET!/PDI_CLK"/>
</symbol>
<symbol name="XMEGA128A1">
<pin name="PF0"/>
<pin name="PF1"/>
<pin name="PF2"/>
<pin name="PF3"/>
<pin name="PF4"/>
<pin name="PF5"/>
<pin name="PF6"/>
<pin name="PF7"/>
<pin name="PE0"/>
<pin name="PE1"/>
<pin name="PE2"/>
<pin name="PE3"/>
<pin name="PE4"/>
<pin name="PE5"/>
<pin name="PE6"/>
<pin name="PE7"/>
<pin name="PD7"/>
<pin name="PD6"/>
<pin name="PD5"/>
<pin name="PD4"/>
<pin name="PD3"/>
<pin name="PD2"/>
<pin name="PD1"/>
<pin name="PD0"/>
<pin name="PC7"/>
<pin name="PC6"/>
<pin name="PC5"/>
<pin name="PC4"/>
<pin name="PC3"/>
<pin name="PC2"/>
<pin name="PC1"/>
<pin name="PC0"/>
<pin name="PB0"/>
<pin name="PA6"/>
<pin name="PA7"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="AVCC1" direction="pwr"/>
<pin name="GND9" direction="pwr"/>
<pin name="PDI_DATA"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET!/PDI_CLK" direction="in"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="GND5" direction="pwr"/>
<pin name="GND6" direction="pwr"/>
<pin name="GND7" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC3" direction="pwr"/>
<pin name="VCC4" direction="pwr"/>
<pin name="VCC5" direction="pwr"/>
<pin name="VCC6" direction="pwr"/>
<pin name="VCC7" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND8" direction="pwr"/>
<pin name="PH0"/>
<pin name="PH1"/>
<pin name="PH2"/>
<pin name="PH3"/>
<pin name="PH4"/>
<pin name="PH5"/>
<pin name="PH6"/>
<pin name="PH7"/>
<pin name="PJ0"/>
<pin name="PJ1"/>
<pin name="PJ2"/>
<pin name="PJ3"/>
<pin name="PJ4"/>
<pin name="PJ5"/>
<pin name="PJ6"/>
<pin name="PJ7"/>
<pin name="PK0"/>
<pin name="PK1"/>
<pin name="PK2"/>
<pin name="PK3"/>
<pin name="PK4"/>
<pin name="PK5"/>
<pin name="PK6"/>
<pin name="PK7"/>
<pin name="PQ0"/>
<pin name="PQ1"/>
<pin name="PQ2"/>
<pin name="PQ3"/>
<pin name="PR0(XT2)"/>
<pin name="PR1(XT1)"/>
<pin name="PB1"/>
<pin name="PB2"/>
<pin name="PB3"/>
<pin name="PB4"/>
<pin name="PB5"/>
<pin name="PB6"/>
<pin name="PB7"/>
</symbol>
<symbol name="ATMEGA325P">
<pin name="DNC" direction="in"/>
<pin name="RXD/PCINT0/PE0"/>
<pin name="TXD/PCINT1/PE1"/>
<pin name="XCK/AIN0/PCINT2/PE2"/>
<pin name="AIN1/PCINT3/PE3"/>
<pin name="USCK/SCL/PCINT4/PE4"/>
<pin name="DI/SDA/PCINT5/PE5"/>
<pin name="DO/PCINT6/PE6"/>
<pin name="CLKO/PCINT7/PE7"/>
<pin name="!SS!/PCINT8/PB0"/>
<pin name="SCK/PCINT9/PB1"/>
<pin name="MOSI/PCINT10/PB2"/>
<pin name="MISO/PCINT11/PB3"/>
<pin name="OC0A/PCINT12/PB4"/>
<pin name="OC1B/PCINT14/PB6"/>
<pin name="OC1A/PCINT13/PB5"/>
<pin name="OC2A/PCINT15/PB7"/>
<pin name="T1/PG3"/>
<pin name="T0/PG4"/>
<pin name="!RESET!/PG5" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TOSC2/XTAL2" direction="out"/>
<pin name="TOSC1/XTAL1" direction="in"/>
<pin name="ICP1/PD0"/>
<pin name="INT0/PD1"/>
<pin name="PD2"/>
<pin name="PD3"/>
<pin name="PD4"/>
<pin name="PD5"/>
<pin name="PD6"/>
<pin name="PD7"/>
<pin name="PG0"/>
<pin name="PG1"/>
<pin name="PC0"/>
<pin name="PC1"/>
<pin name="PC3"/>
<pin name="PC4"/>
<pin name="PC5"/>
<pin name="PC6"/>
<pin name="PC7"/>
<pin name="PG2"/>
<pin name="PC2"/>
<pin name="PA7"/>
<pin name="PA6"/>
<pin name="PA5"/>
<pin name="PA4"/>
<pin name="PA3"/>
<pin name="PA2"/>
<pin name="PA1"/>
<pin name="PA0"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="ADC7/TDI/PF7"/>
<pin name="ADC6/TDO/PF6"/>
<pin name="ADC5/TMS/PF5"/>
<pin name="ADC4/TCK/PF4"/>
<pin name="ADC3/PF3"/>
<pin name="ADC2/PF2"/>
<pin name="ADC1/PF1"/>
<pin name="ADC0/PF0"/>
<pin name="AREF" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="AT45DB642D">
<pin name="SI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="!WP" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="RDY/!BUSY" direction="out"/>
<pin name="I/O3"/>
<pin name="I/O2"/>
<pin name="I/O1"/>
<pin name="I/O0"/>
<pin name="SER/!BYTE" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SCK/CLK" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="I/O7"/>
<pin name="I/O6"/>
<pin name="I/O5"/>
<pin name="I/O4"/>
<pin name="VCCP" direction="pwr"/>
<pin name="GNDP" direction="pwr"/>
</symbol>
<symbol name="ATMEGA644-20PU">
<pin name="PCINT8/XCK0/T0_PB0"/>
<pin name="PCINT9/CLKO/T1_PB1"/>
<pin name="PCINT10/INT2/AIN0_PB2"/>
<pin name="PCINT11/OC0A/AIN1_PB3"/>
<pin name="PCINT12/OC0B/SS_PB4"/>
<pin name="PCINT13/MOSI_PB5"/>
<pin name="PCINT14/MISO_PB6"/>
<pin name="PCINT15/SCK_PB7"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="PCINT24/RXD0_PD0"/>
<pin name="PCINT25/TXD0_PD1"/>
<pin name="PCINT26/INT0_PD2"/>
<pin name="PCINT27/INT1_PD3"/>
<pin name="PCINT28/OC1B_PD4"/>
<pin name="PCINT29/OC1A_PD5"/>
<pin name="PCINT30/OC2B/ICP_PD6"/>
<pin name="PCINT31/OC2A_PD7"/>
<pin name="PCINT16/SCL_PC0"/>
<pin name="PCINT17/SDA_PC1"/>
<pin name="PCINT18/TCK_PC2"/>
<pin name="PCINT19/TMS_PC3"/>
<pin name="PCINT20/TDO_PC4"/>
<pin name="PCINT21/TDI_PC5"/>
<pin name="PCINT22/TOSC1_PC6"/>
<pin name="PCINT23/TOSC2_PC7"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="AREF" direction="pas"/>
<pin name="PCINT7/ADC7_PA7"/>
<pin name="PCINT6/ADC6_PA6"/>
<pin name="PCINT5/ADC5_PA5"/>
<pin name="PCINT4/ADC4_PA4"/>
<pin name="PCINT3/ADC3_PA3"/>
<pin name="PCINT2/ADC2_PA2"/>
<pin name="PCINT1/ADC1_PA1"/>
<pin name="PCINT0/ADC0_PA0"/>
</symbol>
<symbol name="AT45DB161D">
<pin name="!CS" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="!WP" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="RDY/!BUSY" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AT45DB161VFN8">
<pin name="!CS" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="SO" direction="out"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!WP" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="AT90*4434P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC0" pad="22"/>
<connect gate="G$1" pin="PC1" pad="23"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*4434" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (LS)&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-4"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="44"/>
<connect gate="G$1" pin="VCC2" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0" pad="19"/>
<connect gate="G$1" pin="PC1" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*8535P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC0" pad="22"/>
<connect gate="G$1" pin="PC1" pad="23"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*8535" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="32-I/O-4"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AGND" pad="34"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="24"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="PC0" pad="25"/>
<connect gate="G$1" pin="PC1" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VCC1" pad="11"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0" pad="19"/>
<connect gate="G$1" pin="PC1" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S4414" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
256 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="ICP" pad="31"/>
<connect gate="G$1" pin="OC1B" pad="29"/>
<connect gate="G$1" pin="PD4" pad="14"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J1" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J2" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J3" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515-A" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-2"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-2"/>
</gates>
<devices>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="ICP" pad="35"/>
<connect gate="G$1" pin="NC1" pad="34"/>
<connect gate="G$1" pin="NC2" pad="23"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="1"/>
<connect gate="G$1" pin="OC1B" pad="32"/>
<connect gate="G$1" pin="PD4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="ICP" pad="29"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="OC1B" pad="26"/>
<connect gate="G$1" pin="PD4" pad="10"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S8515P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes SRAM&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="32-I/O-1"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="ICP" pad="31"/>
<connect gate="G$1" pin="OC1B" pad="29"/>
<connect gate="G$1" pin="PD4" pad="14"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2333A" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10-bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-1"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(ADC0)PC0" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="10"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(ICP)PB0" pad="12"/>
<connect gate="G$1" pin="(INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(INT1)PD3" pad="1"/>
<connect gate="G$1" pin="(MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1)PB1" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(SS)PB2" pad="14"/>
<connect gate="G$1" pin="(T0)PD4" pad="2"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="31"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="NC3" pad="19"/>
<connect gate="G$1" pin="NC4" pad="22"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2333P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10-bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-2"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="12"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(ICP)PB0" pad="14"/>
<connect gate="G$1" pin="(INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(INT1)PD3" pad="5"/>
<connect gate="G$1" pin="(MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="17"/>
<connect gate="G$1" pin="(OC1)PB1" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(SS)PB2" pad="16"/>
<connect gate="G$1" pin="(T0)PD4" pad="6"/>
<connect gate="G$1" pin="(T1)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S4433" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
4 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
256 bytes EEPROM&lt;p&gt;
UART&lt;p&gt;
6-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="20-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="12"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="13"/>
<connect gate="G$1" pin="(ICP)PB0" pad="14"/>
<connect gate="G$1" pin="(INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(INT1)PD3" pad="5"/>
<connect gate="G$1" pin="(MISO)PB4" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="17"/>
<connect gate="G$1" pin="(OC1)PB1" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB5" pad="19"/>
<connect gate="G$1" pin="(SS)PB2" pad="16"/>
<connect gate="G$1" pin="(T0)PD4" pad="6"/>
<connect gate="G$1" pin="(T1)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="22"/>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(ADC0)PC0)" pad="23"/>
<connect gate="G$1" pin="(ADC1)PC1" pad="24"/>
<connect gate="G$1" pin="(ADC2)PC2" pad="25"/>
<connect gate="G$1" pin="(ADC3)PC3" pad="26"/>
<connect gate="G$1" pin="(ADC4)PC4" pad="27"/>
<connect gate="G$1" pin="(ADC5)PC5" pad="28"/>
<connect gate="G$1" pin="(AIN0)PD6" pad="10"/>
<connect gate="G$1" pin="(AIN1)PD7" pad="11"/>
<connect gate="G$1" pin="(ICP)PB0" pad="12"/>
<connect gate="G$1" pin="(INT0)PD2" pad="32"/>
<connect gate="G$1" pin="(INT1)PD3" pad="1"/>
<connect gate="G$1" pin="(MISO)PB4" pad="16"/>
<connect gate="G$1" pin="(MOSI)PB3" pad="15"/>
<connect gate="G$1" pin="(OC1)PB1" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="30"/>
<connect gate="G$1" pin="(SCK)PB5" pad="17"/>
<connect gate="G$1" pin="(SS)PB2" pad="14"/>
<connect gate="G$1" pin="(T0)PD4" pad="2"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="31"/>
<connect gate="G$1" pin="AGND" pad="21"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*2323" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="3-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="XTAL1" pad="2"/>
<connect gate="G$1" pin="XTAL2" pad="3"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90*2343" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="5-I/O-1"/>
</gates>
<devices>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S2313" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
128 bytes SRAM&lt;p&gt;
128 bytes EEPROM&lt;p&gt;
UART</description>
<gates>
<gate name="G$1" symbol="15-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(OCI)PB3" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(ICP)PD6" pad="11"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(INT1)PD3" pad="7"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(OCI)PB3" pad="15"/>
<connect gate="G$1" pin="(RXD)PD0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="(T1)PD5" pad="9"/>
<connect gate="G$1" pin="(TXD)PD1" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="V" package="MLF20-4X4">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="10"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="11"/>
<connect gate="G$1" pin="(ICP)PD6" pad="9"/>
<connect gate="G$1" pin="(INT0)PD2" pad="4"/>
<connect gate="G$1" pin="(INT1)PD3" pad="5"/>
<connect gate="G$1" pin="(MISO)PB6" pad="16"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="15"/>
<connect gate="G$1" pin="(OCI)PB3" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="20"/>
<connect gate="G$1" pin="(SCK)PB7" pad="17"/>
<connect gate="G$1" pin="(T0)PD4" pad="6"/>
<connect gate="G$1" pin="(T1)PD5" pad="7"/>
<connect gate="G$1" pin="(TXD)PD1" pad="1"/>
<connect gate="G$1" pin="GND" pad="8 TH" route="any"/>
<connect gate="G$1" pin="PB2" pad="12"/>
<connect gate="G$1" pin="PB4" pad="14"/>
<connect gate="G$1" pin="RESET" pad="19"/>
<connect gate="G$1" pin="VCC" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="3"/>
<connect gate="G$1" pin="XTAL2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90S1200" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="15-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="Y" package="SSOP20D8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="12"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="13"/>
<connect gate="G$1" pin="(INT0)PD2" pad="6"/>
<connect gate="G$1" pin="(MISO)PB6" pad="18"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="17"/>
<connect gate="G$1" pin="(SCK)PB7" pad="19"/>
<connect gate="G$1" pin="(T0)PD4" pad="8"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="PB2" pad="14"/>
<connect gate="G$1" pin="PB3" pad="15"/>
<connect gate="G$1" pin="PB4" pad="16"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD3" pad="7"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="11"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY10" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes ROM</description>
<gates>
<gate name="G$1" symbol="6-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY11*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="6-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(AIN0)PB0" pad="5"/>
<connect gate="G$1" pin="(AIN1)PB1" pad="6"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(T0)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="3617970"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="3617970"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY12*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="6-I/O-2"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(RESET)PB5" pad="1"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="(XTAL1)PB3" pad="2"/>
<connect gate="G$1" pin="(XTAL2)PB4" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY22" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1K ROM&lt;p&gt;
128 bytes RAM&lt;p&gt;
128 bytes EEPROM</description>
<gates>
<gate name="G$1" symbol="5-I/O-1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(CLOCK)PB3" pad="2"/>
<connect gate="G$1" pin="(MISO)PB1" pad="6"/>
<connect gate="G$1" pin="(MOSI)PB0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB2" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB4" pad="3"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA103*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (L)&lt;br&gt;
128 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
2 Kbytes EEPROM&lt;br&gt;
UART&lt;br&gt;
RTC&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="48-I/O-1"/>
</gates>
<devices>
<device name="" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AC+)PE2" pad="4"/>
<connect gate="G$1" pin="(AC-)PE3" pad="5"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(TXD)PE1" pad="3"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="ALE" pad="43"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7)" pad="54"/>
<connect gate="G$1" pin="RD" pad="34"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="TOSC1" pad="19"/>
<connect gate="G$1" pin="TOSC2" pad="18"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="WR" pad="33"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT90C8534" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;p&gt;
512 bytes EEPROM&lt;p&gt;
256 bytes SRAM&lt;p&gt;
6-channel&lt;p&gt;
10-bit A/D</description>
<gates>
<gate name="G$1" symbol="15-I/O-3"/>
</gates>
<devices>
<device name="A" package="TQFP48">
<connects>
<connect gate="G$1" pin="ADIN0" pad="1"/>
<connect gate="G$1" pin="ADIN1" pad="13"/>
<connect gate="G$1" pin="ADIN2" pad="14"/>
<connect gate="G$1" pin="ADIN3" pad="15"/>
<connect gate="G$1" pin="ADIN4" pad="16"/>
<connect gate="G$1" pin="ADIN5" pad="17"/>
<connect gate="G$1" pin="AGND" pad="11"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="31"/>
<connect gate="G$1" pin="INT0" pad="35"/>
<connect gate="G$1" pin="INT1" pad="34"/>
<connect gate="G$1" pin="NC1" pad="2"/>
<connect gate="G$1" pin="NC10" pad="12"/>
<connect gate="G$1" pin="NC11" pad="19"/>
<connect gate="G$1" pin="NC12" pad="21"/>
<connect gate="G$1" pin="NC13" pad="25"/>
<connect gate="G$1" pin="NC14" pad="26"/>
<connect gate="G$1" pin="NC15" pad="27"/>
<connect gate="G$1" pin="NC16" pad="28"/>
<connect gate="G$1" pin="NC17" pad="29"/>
<connect gate="G$1" pin="NC18" pad="30"/>
<connect gate="G$1" pin="NC19" pad="32"/>
<connect gate="G$1" pin="NC2" pad="3"/>
<connect gate="G$1" pin="NC20" pad="36"/>
<connect gate="G$1" pin="NC21" pad="37"/>
<connect gate="G$1" pin="NC22" pad="40"/>
<connect gate="G$1" pin="NC23" pad="41"/>
<connect gate="G$1" pin="NC24" pad="42"/>
<connect gate="G$1" pin="NC25" pad="43"/>
<connect gate="G$1" pin="NC26" pad="48"/>
<connect gate="G$1" pin="NC3" pad="4"/>
<connect gate="G$1" pin="NC4" pad="5"/>
<connect gate="G$1" pin="NC5" pad="6"/>
<connect gate="G$1" pin="NC6" pad="7"/>
<connect gate="G$1" pin="NC7" pad="8"/>
<connect gate="G$1" pin="NC8" pad="9"/>
<connect gate="G$1" pin="NC9" pad="10"/>
<connect gate="G$1" pin="PA0" pad="47"/>
<connect gate="G$1" pin="PA1" pad="46"/>
<connect gate="G$1" pin="PA2" pad="45"/>
<connect gate="G$1" pin="PA3" pad="44"/>
<connect gate="G$1" pin="PA4" pad="39"/>
<connect gate="G$1" pin="PA5" pad="38"/>
<connect gate="G$1" pin="PA6" pad="33"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA161*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
dual UART&lt;br&gt;
hardware multiplier&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="35-I/O-1"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(ALE)PE1" pad="30"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(INT2)PE0" pad="31"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="29"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="10"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="3"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="14"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="15"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="11"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="4"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16PU"/>
<attribute name="OC_FARNELL" value="9171142"/>
<attribute name="OC_NEWARK" value="98M0167"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16PU"/>
<attribute name="OC_FARNELL" value="9171142"/>
<attribute name="OC_NEWARK" value="98M0167"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA161*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
dual UART&lt;br&gt;
hardware multiplier&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="35-I/O-2"/>
</gates>
<devices>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-S" package="S44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J-SM" package="PLCC-SM44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(ALE)PE1" pad="33"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(INT2)PE0" pad="35"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="32"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="11"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="4"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="16"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="17"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="13"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="5"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(ALE)PE1" pad="27"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(INT2)PE0" pad="29"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1B)PE2" pad="26"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD0)PD0" pad="5"/>
<connect gate="G$1" pin="(RXD1)PB2" pad="42"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PD4" pad="10"/>
<connect gate="G$1" pin="(TOSC2)PD5" pad="11"/>
<connect gate="G$1" pin="(TXD0)PD1" pad="7"/>
<connect gate="G$1" pin="(TXD1)PB3" pad="43"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16AU"/>
<attribute name="OC_FARNELL" value="9171134"/>
<attribute name="OC_NEWARK" value="96K6515"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY15L" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2.7 V&lt;p&gt;
1 Kbytes FLASH&lt;p&gt;
64 bytes EEPROM&lt;p&gt;
4-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="6-I/O-3"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="(ADC0)PB5" pad="1"/>
<connect gate="G$1" pin="(ADC1)PB2" pad="7"/>
<connect gate="G$1" pin="(ADC2)PB3" pad="3"/>
<connect gate="G$1" pin="(ADC3)PB4" pad="2"/>
<connect gate="G$1" pin="(AREF)PB0" pad="5"/>
<connect gate="G$1" pin="(OCP)PB1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="(ADC0)PB5" pad="1"/>
<connect gate="G$1" pin="(ADC1)PB2" pad="7"/>
<connect gate="G$1" pin="(ADC2)PB3" pad="3"/>
<connect gate="G$1" pin="(ADC3)PB4" pad="2"/>
<connect gate="G$1" pin="(AREF)PB0" pad="5"/>
<connect gate="G$1" pin="(OCP)PB1" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA163*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 Kbytes &lt;B&gt;EEPROM&lt;/B&gt;&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
UART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
hardware multiplier&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-5"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA163*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
UART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
hardware multiplier&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-6"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY28*P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1.8 V&lt;p&gt;
2 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="20-I/O-3"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="(IR)PA2" pad="25"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND1" pad="22"/>
<connect gate="G$1" pin="NC1" pad="21"/>
<connect gate="G$1" pin="PA0" pad="28"/>
<connect gate="G$1" pin="PA1" pad="27"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PB0(AIN0)" pad="14"/>
<connect gate="G$1" pin="PB1(AIN1)" pad="15"/>
<connect gate="G$1" pin="PB2(T0)" pad="16"/>
<connect gate="G$1" pin="PB3(INT0)" pad="17"/>
<connect gate="G$1" pin="PB4(INT1)" pad="18"/>
<connect gate="G$1" pin="PB5" pad="19"/>
<connect gate="G$1" pin="PB6" pad="23"/>
<connect gate="G$1" pin="PB7" pad="24"/>
<connect gate="G$1" pin="PD0" pad="2"/>
<connect gate="G$1" pin="PD1" pad="3"/>
<connect gate="G$1" pin="PD2" pad="4"/>
<connect gate="G$1" pin="PD3" pad="5"/>
<connect gate="G$1" pin="PD4" pad="6"/>
<connect gate="G$1" pin="PD5" pad="11"/>
<connect gate="G$1" pin="PD6" pad="12"/>
<connect gate="G$1" pin="PD7" pad="13"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
</connects>
<technologies>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY28*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
1.8 V&lt;p&gt;
2 Kbytes FLASH</description>
<gates>
<gate name="G$1" symbol="20-I/O-4"/>
</gates>
<devices>
<device name="A" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="(IR)PA2" pad="25"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND1" pad="21"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="6"/>
<connect gate="G$1" pin="NC3" pad="19"/>
<connect gate="G$1" pin="NC4" pad="20"/>
<connect gate="G$1" pin="NC5" pad="22"/>
<connect gate="G$1" pin="PA0" pad="28"/>
<connect gate="G$1" pin="PA1" pad="27"/>
<connect gate="G$1" pin="PA3" pad="26"/>
<connect gate="G$1" pin="PB0(AIN0)" pad="12"/>
<connect gate="G$1" pin="PB1(AIN1)" pad="13"/>
<connect gate="G$1" pin="PB2(T0)" pad="14"/>
<connect gate="G$1" pin="PB3(INT0)" pad="15"/>
<connect gate="G$1" pin="PB4(INT1)" pad="16"/>
<connect gate="G$1" pin="PB5" pad="17"/>
<connect gate="G$1" pin="PB6" pad="23"/>
<connect gate="G$1" pin="PB7" pad="24"/>
<connect gate="G$1" pin="PD0" pad="30"/>
<connect gate="G$1" pin="PD1" pad="31"/>
<connect gate="G$1" pin="PD2" pad="32"/>
<connect gate="G$1" pin="PD3" pad="1"/>
<connect gate="G$1" pin="PD4" pad="2"/>
<connect gate="G$1" pin="PD5" pad="9"/>
<connect gate="G$1" pin="PD6" pad="10"/>
<connect gate="G$1" pin="PD7" pad="11"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VCC1" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
</connects>
<technologies>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT25*" prefix="IC">
<description>SPI bus serial &lt;B&gt;EEPROM&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="250X0"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CS/" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="HOLD/" pad="7"/>
<connect gate="G$1" pin="SCK" pad="6"/>
<connect gate="G$1" pin="SI" pad="5"/>
<connect gate="G$1" pin="SO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP/" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CAT25040LI-G"/>
<attribute name="OC_FARNELL" value="1718045"/>
<attribute name="OC_NEWARK" value="06R0588"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT24C*" prefix="IC">
<description>2-wire serial &lt;B&gt;EEPROM&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="24CXX"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT24C1024BW-SH-B"/>
<attribute name="OC_FARNELL" value="1362646"/>
<attribute name="OC_NEWARK" value="03P2044"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDE2506" prefix="IC">
<description>I2C/MicroWire &lt;B&gt;EEPROM&lt;/B&gt; (24xxx)</description>
<gates>
<gate name="G$1" symbol="SDE2506"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CE/" pad="2"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="TG" pad="8"/>
<connect gate="G$1" pin="TP" pad="7"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT93C*6" prefix="IC">
<description>3-wire serial EEPROM</description>
<gates>
<gate name="G$1" symbol="93CX6"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DC" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ORG" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT93C46D-PU"/>
<attribute name="OC_FARNELL" value="1362666"/>
<attribute name="OC_NEWARK" value="50M3339"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C2051" prefix="IC">
<description>80C31 &lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
2 Kbytes FLASH&lt;p&gt;
2.7 V</description>
<gates>
<gate name="G$1" symbol="89C2051"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="AIN0-P1.0" pad="12"/>
<connect gate="G$1" pin="AIN1-P1.1" pad="13"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="P1.2" pad="14"/>
<connect gate="G$1" pin="P1.3" pad="15"/>
<connect gate="G$1" pin="P1.4" pad="16"/>
<connect gate="G$1" pin="P1.5" pad="17"/>
<connect gate="G$1" pin="P1.6" pad="18"/>
<connect gate="G$1" pin="P1.7" pad="19"/>
<connect gate="G$1" pin="P3.0-RXD" pad="2"/>
<connect gate="G$1" pin="P3.1-TXD" pad="3"/>
<connect gate="G$1" pin="P3.2-INTO/" pad="6"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="7"/>
<connect gate="G$1" pin="P3.4-T0" pad="8"/>
<connect gate="G$1" pin="P3.5-T1" pad="9"/>
<connect gate="G$1" pin="P3.7" pad="11"/>
<connect gate="G$1" pin="RST-VPP" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C2051-12PU"/>
<attribute name="OC_FARNELL" value="1699389"/>
<attribute name="OC_NEWARK" value="80P3687"/>
</technology>
</technologies>
</device>
<device name="S" package="SOIC20S">
<connects>
<connect gate="G$1" pin="AIN0-P1.0" pad="12"/>
<connect gate="G$1" pin="AIN1-P1.1" pad="13"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="P1.2" pad="14"/>
<connect gate="G$1" pin="P1.3" pad="15"/>
<connect gate="G$1" pin="P1.4" pad="16"/>
<connect gate="G$1" pin="P1.5" pad="17"/>
<connect gate="G$1" pin="P1.6" pad="18"/>
<connect gate="G$1" pin="P1.7" pad="19"/>
<connect gate="G$1" pin="P3.0-RXD" pad="2"/>
<connect gate="G$1" pin="P3.1-TXD" pad="3"/>
<connect gate="G$1" pin="P3.2-INTO/" pad="6"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="7"/>
<connect gate="G$1" pin="P3.4-T0" pad="8"/>
<connect gate="G$1" pin="P3.5-T1" pad="9"/>
<connect gate="G$1" pin="P3.7" pad="11"/>
<connect gate="G$1" pin="RST-VPP" pad="1"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C2051-12SU"/>
<attribute name="OC_FARNELL" value="1699390"/>
<attribute name="OC_NEWARK" value="80P3688"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA103*" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Low-voltage (L)&lt;p&gt;
128 Kbytes FLASH&lt;p&gt;
4 Kbytes SRAM&lt;p&gt;
2 Kbytes EEPROM&lt;p&gt;
UART&lt;p&gt;
RTC&lt;p&gt;
8-channel 10 bit ADC</description>
<gates>
<gate name="G$1" symbol="48-I/O-2"/>
</gates>
<devices>
<device name="" package="TQFP64">
<connects>
<connect gate="G$1" pin="01" pad="21"/>
<connect gate="G$1" pin="02" pad="22"/>
<connect gate="G$1" pin="A10-PC2" pad="37"/>
<connect gate="G$1" pin="A11-PC3" pad="38"/>
<connect gate="G$1" pin="A12-PC4" pad="39"/>
<connect gate="G$1" pin="A13-PC5" pad="40"/>
<connect gate="G$1" pin="A14-PC6" pad="41"/>
<connect gate="G$1" pin="A15-PC7" pad="42"/>
<connect gate="G$1" pin="A8-PC0" pad="35"/>
<connect gate="G$1" pin="A9-PC1" pad="36"/>
<connect gate="G$1" pin="AC+_PE2" pad="4"/>
<connect gate="G$1" pin="AC-_PE3" pad="5"/>
<connect gate="G$1" pin="AD0-PA0" pad="51"/>
<connect gate="G$1" pin="AD1-PA1" pad="50"/>
<connect gate="G$1" pin="AD2-PA2" pad="49"/>
<connect gate="G$1" pin="AD3-PA3" pad="48"/>
<connect gate="G$1" pin="AD4-PA4" pad="47"/>
<connect gate="G$1" pin="AD5-PA5" pad="46"/>
<connect gate="G$1" pin="AD6-PA6" pad="45"/>
<connect gate="G$1" pin="AD7-PA7" pad="44"/>
<connect gate="G$1" pin="ADC0-PF0" pad="61"/>
<connect gate="G$1" pin="ADC1-PF1" pad="60"/>
<connect gate="G$1" pin="ADC2-PF2" pad="59"/>
<connect gate="G$1" pin="ADC3-PF3" pad="58"/>
<connect gate="G$1" pin="ADC4-PF4" pad="57"/>
<connect gate="G$1" pin="ADC5-PF5" pad="56"/>
<connect gate="G$1" pin="ADC6-PF6" pad="55"/>
<connect gate="G$1" pin="ADC7-PF7" pad="54"/>
<connect gate="G$1" pin="AGND" pad="63"/>
<connect gate="G$1" pin="ALE" pad="43"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="AVREF" pad="62"/>
<connect gate="G$1" pin="GND" pad="53"/>
<connect gate="G$1" pin="INT4-PE4" pad="6"/>
<connect gate="G$1" pin="INT5-PE5" pad="7"/>
<connect gate="G$1" pin="INT6-PE6" pad="8"/>
<connect gate="G$1" pin="INT7-PE7" pad="9"/>
<connect gate="G$1" pin="MISO-PB3" pad="13"/>
<connect gate="G$1" pin="MOSI-PB2" pad="12"/>
<connect gate="G$1" pin="OC0-PB4" pad="14"/>
<connect gate="G$1" pin="OC1A-PB5" pad="15"/>
<connect gate="G$1" pin="OC1B-PB6" pad="16"/>
<connect gate="G$1" pin="OC2-PB7" pad="17"/>
<connect gate="G$1" pin="PD0-INT0" pad="25"/>
<connect gate="G$1" pin="PD1-INT1" pad="26"/>
<connect gate="G$1" pin="PD2-INT2" pad="27"/>
<connect gate="G$1" pin="PD3-INT3" pad="28"/>
<connect gate="G$1" pin="PD4-IC1" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6-T1" pad="31"/>
<connect gate="G$1" pin="PD7-T2" pad="32"/>
<connect gate="G$1" pin="PEN/" pad="1"/>
<connect gate="G$1" pin="RD/" pad="34"/>
<connect gate="G$1" pin="RESET/" pad="20"/>
<connect gate="G$1" pin="RXD-PE0" pad="2"/>
<connect gate="G$1" pin="SCK-PB1" pad="11"/>
<connect gate="G$1" pin="SS-PB0" pad="10"/>
<connect gate="G$1" pin="TOSC1" pad="19"/>
<connect gate="G$1" pin="TOSC2" pad="18"/>
<connect gate="G$1" pin="TXD-PE1" pad="3"/>
<connect gate="G$1" pin="VCC" pad="52"/>
<connect gate="G$1" pin="WR/" pad="33"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C*52" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH; 2K Bytes EEPROM&lt;br&gt;
Compatible with MCS-51 Products&lt;br&gt;
at89s8252.pdf</description>
<gates>
<gate name="G$1" symbol="AT89C52"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="P6" package="DIL40">
<connects>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="EA" pad="31"/>
<connect gate="G$1" pin="P0.0AD0" pad="39"/>
<connect gate="G$1" pin="P0.1AD1" pad="38"/>
<connect gate="G$1" pin="P0.2AD2" pad="37"/>
<connect gate="G$1" pin="P0.3AD3" pad="36"/>
<connect gate="G$1" pin="P0.4AD4" pad="35"/>
<connect gate="G$1" pin="P0.5AD5" pad="34"/>
<connect gate="G$1" pin="P0.6AD6" pad="33"/>
<connect gate="G$1" pin="P0.7AD7" pad="32"/>
<connect gate="G$1" pin="P1.0_T2" pad="1"/>
<connect gate="G$1" pin="P1.1_T2EX" pad="2"/>
<connect gate="G$1" pin="P1.2" pad="3"/>
<connect gate="G$1" pin="P1.3" pad="4"/>
<connect gate="G$1" pin="P1.4" pad="5"/>
<connect gate="G$1" pin="P1.5" pad="6"/>
<connect gate="G$1" pin="P1.6" pad="7"/>
<connect gate="G$1" pin="P1.7" pad="8"/>
<connect gate="G$1" pin="P2.0_A8" pad="21"/>
<connect gate="G$1" pin="P2.1_A9" pad="22"/>
<connect gate="G$1" pin="P2.2_A10" pad="23"/>
<connect gate="G$1" pin="P2.3_A11" pad="24"/>
<connect gate="G$1" pin="P2.4_A12" pad="25"/>
<connect gate="G$1" pin="P2.5_A13" pad="26"/>
<connect gate="G$1" pin="P2.6_A14" pad="27"/>
<connect gate="G$1" pin="P2.7_A15" pad="28"/>
<connect gate="G$1" pin="P3.0" pad="10"/>
<connect gate="G$1" pin="P3.1" pad="11"/>
<connect gate="G$1" pin="P3.2" pad="12"/>
<connect gate="G$1" pin="P3.3" pad="13"/>
<connect gate="G$1" pin="P3.4/T0" pad="14"/>
<connect gate="G$1" pin="P3.5/T1" pad="15"/>
<connect gate="G$1" pin="P3.6/WR" pad="16"/>
<connect gate="G$1" pin="P3.7/RD" pad="17"/>
<connect gate="G$1" pin="PSEN" pad="29"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="EA" pad="35"/>
<connect gate="G$1" pin="P0.0AD0" pad="43"/>
<connect gate="G$1" pin="P0.1AD1" pad="42"/>
<connect gate="G$1" pin="P0.2AD2" pad="41"/>
<connect gate="G$1" pin="P0.3AD3" pad="40"/>
<connect gate="G$1" pin="P0.4AD4" pad="39"/>
<connect gate="G$1" pin="P0.5AD5" pad="38"/>
<connect gate="G$1" pin="P0.6AD6" pad="37"/>
<connect gate="G$1" pin="P0.7AD7" pad="36"/>
<connect gate="G$1" pin="P1.0_T2" pad="2"/>
<connect gate="G$1" pin="P1.1_T2EX" pad="3"/>
<connect gate="G$1" pin="P1.2" pad="4"/>
<connect gate="G$1" pin="P1.3" pad="5"/>
<connect gate="G$1" pin="P1.4" pad="6"/>
<connect gate="G$1" pin="P1.5" pad="7"/>
<connect gate="G$1" pin="P1.6" pad="8"/>
<connect gate="G$1" pin="P1.7" pad="9"/>
<connect gate="G$1" pin="P2.0_A8" pad="24"/>
<connect gate="G$1" pin="P2.1_A9" pad="25"/>
<connect gate="G$1" pin="P2.2_A10" pad="26"/>
<connect gate="G$1" pin="P2.3_A11" pad="27"/>
<connect gate="G$1" pin="P2.4_A12" pad="28"/>
<connect gate="G$1" pin="P2.5_A13" pad="29"/>
<connect gate="G$1" pin="P2.6_A14" pad="30"/>
<connect gate="G$1" pin="P2.7_A15" pad="31"/>
<connect gate="G$1" pin="P3.0" pad="11"/>
<connect gate="G$1" pin="P3.1" pad="13"/>
<connect gate="G$1" pin="P3.2" pad="14"/>
<connect gate="G$1" pin="P3.3" pad="15"/>
<connect gate="G$1" pin="P3.4/T0" pad="16"/>
<connect gate="G$1" pin="P3.5/T1" pad="17"/>
<connect gate="G$1" pin="P3.6/WR" pad="18"/>
<connect gate="G$1" pin="P3.7/RD" pad="19"/>
<connect gate="G$1" pin="PSEN" pad="32"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="VCC" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="Q" package="PQFP44">
<connects>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="EA" pad="29"/>
<connect gate="G$1" pin="P0.0AD0" pad="37"/>
<connect gate="G$1" pin="P0.1AD1" pad="36"/>
<connect gate="G$1" pin="P0.2AD2" pad="35"/>
<connect gate="G$1" pin="P0.3AD3" pad="34"/>
<connect gate="G$1" pin="P0.4AD4" pad="33"/>
<connect gate="G$1" pin="P0.5AD5" pad="32"/>
<connect gate="G$1" pin="P0.6AD6" pad="31"/>
<connect gate="G$1" pin="P0.7AD7" pad="30"/>
<connect gate="G$1" pin="P1.0_T2" pad="40"/>
<connect gate="G$1" pin="P1.1_T2EX" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5" pad="1"/>
<connect gate="G$1" pin="P1.6" pad="2"/>
<connect gate="G$1" pin="P1.7" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0" pad="5"/>
<connect gate="G$1" pin="P3.1" pad="7"/>
<connect gate="G$1" pin="P3.2" pad="8"/>
<connect gate="G$1" pin="P3.3" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/WR" pad="12"/>
<connect gate="G$1" pin="P3.7/RD" pad="13"/>
<connect gate="G$1" pin="PSEN" pad="26"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="EA" pad="29"/>
<connect gate="G$1" pin="P0.0AD0" pad="37"/>
<connect gate="G$1" pin="P0.1AD1" pad="36"/>
<connect gate="G$1" pin="P0.2AD2" pad="35"/>
<connect gate="G$1" pin="P0.3AD3" pad="34"/>
<connect gate="G$1" pin="P0.4AD4" pad="33"/>
<connect gate="G$1" pin="P0.5AD5" pad="32"/>
<connect gate="G$1" pin="P0.6AD6" pad="31"/>
<connect gate="G$1" pin="P0.7AD7" pad="30"/>
<connect gate="G$1" pin="P1.0_T2" pad="40"/>
<connect gate="G$1" pin="P1.1_T2EX" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5" pad="1"/>
<connect gate="G$1" pin="P1.6" pad="2"/>
<connect gate="G$1" pin="P1.7" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0" pad="5"/>
<connect gate="G$1" pin="P3.1" pad="7"/>
<connect gate="G$1" pin="P3.2" pad="8"/>
<connect gate="G$1" pin="P3.3" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/WR" pad="12"/>
<connect gate="G$1" pin="P3.7/RD" pad="13"/>
<connect gate="G$1" pin="PSEN" pad="26"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="82">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="27C080" prefix="IC">
<description>&lt;b&gt;8-Megabit (1Mx8) OTP EPROM&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="27C080"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="32P6" package="DIL32">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE!VPP" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A19" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="O0" pad="13"/>
<connect gate="G$1" pin="O1" pad="14"/>
<connect gate="G$1" pin="O2" pad="15"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="18"/>
<connect gate="G$1" pin="O5" pad="19"/>
<connect gate="G$1" pin="O6" pad="20"/>
<connect gate="G$1" pin="O7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT27C080-90PU"/>
<attribute name="OC_FARNELL" value="1455026"/>
<attribute name="OC_NEWARK" value="58M3824"/>
</technology>
</technologies>
</device>
<device name="R" package="SO32X">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE!VPP" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A19" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="O0" pad="13"/>
<connect gate="G$1" pin="O1" pad="14"/>
<connect gate="G$1" pin="O2" pad="15"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="18"/>
<connect gate="G$1" pin="O5" pad="19"/>
<connect gate="G$1" pin="O6" pad="20"/>
<connect gate="G$1" pin="O7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC32R">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="!OE!VPP" pad="24"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="29"/>
<connect gate="G$1" pin="A15" pad="3"/>
<connect gate="G$1" pin="A16" pad="2"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A19" pad="1"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="9"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="6"/>
<connect gate="G$1" pin="A7" pad="5"/>
<connect gate="G$1" pin="A8" pad="27"/>
<connect gate="G$1" pin="A9" pad="26"/>
<connect gate="G$1" pin="O0" pad="13"/>
<connect gate="G$1" pin="O1" pad="14"/>
<connect gate="G$1" pin="O2" pad="15"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="18"/>
<connect gate="G$1" pin="O5" pad="19"/>
<connect gate="G$1" pin="O6" pad="20"/>
<connect gate="G$1" pin="O7" pad="21"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT27C080-90JU"/>
<attribute name="OC_FARNELL" value="1455025"/>
<attribute name="OC_NEWARK" value="58M3823"/>
</technology>
</technologies>
</device>
<device name="T" package="TSOP32">
<connects>
<connect gate="G$1" pin="!CE" pad="30"/>
<connect gate="G$1" pin="!OE!VPP" pad="32"/>
<connect gate="G$1" pin="A0" pad="20"/>
<connect gate="G$1" pin="A1" pad="19"/>
<connect gate="G$1" pin="A10" pad="31"/>
<connect gate="G$1" pin="A11" pad="1"/>
<connect gate="G$1" pin="A12" pad="12"/>
<connect gate="G$1" pin="A13" pad="4"/>
<connect gate="G$1" pin="A14" pad="5"/>
<connect gate="G$1" pin="A15" pad="11"/>
<connect gate="G$1" pin="A16" pad="10"/>
<connect gate="G$1" pin="A17" pad="6"/>
<connect gate="G$1" pin="A18" pad="7"/>
<connect gate="G$1" pin="A19" pad="9"/>
<connect gate="G$1" pin="A2" pad="18"/>
<connect gate="G$1" pin="A3" pad="17"/>
<connect gate="G$1" pin="A4" pad="16"/>
<connect gate="G$1" pin="A5" pad="15"/>
<connect gate="G$1" pin="A6" pad="14"/>
<connect gate="G$1" pin="A7" pad="13"/>
<connect gate="G$1" pin="A8" pad="3"/>
<connect gate="G$1" pin="A9" pad="2"/>
<connect gate="G$1" pin="O0" pad="21"/>
<connect gate="G$1" pin="O1" pad="22"/>
<connect gate="G$1" pin="O2" pad="23"/>
<connect gate="G$1" pin="O3" pad="25"/>
<connect gate="G$1" pin="O4" pad="26"/>
<connect gate="G$1" pin="O5" pad="27"/>
<connect gate="G$1" pin="O6" pad="28"/>
<connect gate="G$1" pin="O7" pad="29"/>
<connect gate="P" pin="GND" pad="24"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91R4008" prefix="IC">
<description>&lt;b&gt;AT91 ARM® Thumb® RISC-Controller&lt;/b&gt;&lt;p&gt;
Microcontroller AT91R40008</description>
<gates>
<gate name="A" symbol="AT91R4008"/>
<gate name="B" symbol="AT91R4008-PARPORT"/>
<gate name="C" symbol="AT91R4008-ADR"/>
<gate name="D" symbol="D0-15"/>
<gate name="P1" symbol="GND"/>
<gate name="P2" symbol="GND"/>
<gate name="P3" symbol="GND"/>
<gate name="P4" symbol="GND"/>
<gate name="P5" symbol="GND"/>
<gate name="P15" symbol="VDDIO"/>
<gate name="P16" symbol="VDDIO"/>
<gate name="P17" symbol="VDDIO"/>
<gate name="P6" symbol="GND"/>
<gate name="P7" symbol="GND"/>
<gate name="P8" symbol="GND"/>
<gate name="P9" symbol="GND"/>
<gate name="P10" symbol="VDDIO"/>
<gate name="P11" symbol="VDDIO"/>
<gate name="P12" symbol="VDDCORE"/>
<gate name="P13" symbol="VDDCORE"/>
<gate name="P14" symbol="VDDCORE"/>
<gate name="P18" symbol="VDDIO"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="A" pin="GND" pad="78"/>
<connect gate="A" pin="MCKI" pad="82"/>
<connect gate="A" pin="NCS0" pad="97"/>
<connect gate="A" pin="NCS1" pad="98"/>
<connect gate="A" pin="NRD/NOE" pad="92"/>
<connect gate="A" pin="NRST" pad="79"/>
<connect gate="A" pin="NRW0/NWE" pad="93"/>
<connect gate="A" pin="NRW1/NUB" pad="77"/>
<connect gate="A" pin="NWAIT" pad="96"/>
<connect gate="A" pin="NWDOVF" pad="80"/>
<connect gate="A" pin="TCK" pad="91"/>
<connect gate="A" pin="TDI" pad="89"/>
<connect gate="A" pin="TDO" pad="90"/>
<connect gate="A" pin="TMS" pad="88"/>
<connect gate="B" pin="P0/TCLK0" pad="49"/>
<connect gate="B" pin="P1/TIOA0" pad="50"/>
<connect gate="B" pin="P10/IRQ1" pad="63"/>
<connect gate="B" pin="P11/IRQ2" pad="64"/>
<connect gate="B" pin="P12/FIQ" pad="66"/>
<connect gate="B" pin="P13/SCK0" pad="67"/>
<connect gate="B" pin="P14/TXD0" pad="68"/>
<connect gate="B" pin="P15/RXD0" pad="69"/>
<connect gate="B" pin="P16" pad="70"/>
<connect gate="B" pin="P17" pad="71"/>
<connect gate="B" pin="P18" pad="72"/>
<connect gate="B" pin="P19" pad="73"/>
<connect gate="B" pin="P2/TIOB0" pad="51"/>
<connect gate="B" pin="P20/SCK1" pad="74"/>
<connect gate="B" pin="P21/TXD1/NTRI" pad="75"/>
<connect gate="B" pin="P22/RXD1" pad="76"/>
<connect gate="B" pin="P23" pad="83"/>
<connect gate="B" pin="P24/BMS" pad="84"/>
<connect gate="B" pin="P25/MCKO" pad="85"/>
<connect gate="B" pin="P26/NCS2" pad="99"/>
<connect gate="B" pin="P27/NCS3" pad="100"/>
<connect gate="B" pin="P3/TCLK1" pad="54"/>
<connect gate="B" pin="P4/TIOA1" pad="55"/>
<connect gate="B" pin="P5/TIOB1" pad="56"/>
<connect gate="B" pin="P6/TCLK2" pad="57"/>
<connect gate="B" pin="P7/TIOA2" pad="58"/>
<connect gate="B" pin="P8/TIOB2" pad="59"/>
<connect gate="B" pin="P9/IRQ0" pad="60"/>
<connect gate="C" pin="A1" pad="3"/>
<connect gate="C" pin="A10" pad="13"/>
<connect gate="C" pin="A11" pad="14"/>
<connect gate="C" pin="A12" pad="15"/>
<connect gate="C" pin="A13" pad="16"/>
<connect gate="C" pin="A14" pad="17"/>
<connect gate="C" pin="A15" pad="20"/>
<connect gate="C" pin="A16" pad="21"/>
<connect gate="C" pin="A17" pad="22"/>
<connect gate="C" pin="A18" pad="23"/>
<connect gate="C" pin="A19" pad="24"/>
<connect gate="C" pin="A2" pad="4"/>
<connect gate="C" pin="A3" pad="5"/>
<connect gate="C" pin="A4" pad="6"/>
<connect gate="C" pin="A5" pad="7"/>
<connect gate="C" pin="A6" pad="8"/>
<connect gate="C" pin="A7" pad="9"/>
<connect gate="C" pin="A8" pad="11"/>
<connect gate="C" pin="A9" pad="12"/>
<connect gate="C" pin="NLB/A0" pad="1"/>
<connect gate="C" pin="P28/CS7/A20" pad="25"/>
<connect gate="C" pin="P29/CS6/A21" pad="26"/>
<connect gate="C" pin="P30/CS5/A22" pad="29"/>
<connect gate="C" pin="P31/CS4/A23" pad="30"/>
<connect gate="D" pin="D0" pad="31"/>
<connect gate="D" pin="D1" pad="32"/>
<connect gate="D" pin="D10" pad="42"/>
<connect gate="D" pin="D11" pad="43"/>
<connect gate="D" pin="D12" pad="45"/>
<connect gate="D" pin="D13" pad="46"/>
<connect gate="D" pin="D14" pad="47"/>
<connect gate="D" pin="D15" pad="48"/>
<connect gate="D" pin="D2" pad="33"/>
<connect gate="D" pin="D3" pad="34"/>
<connect gate="D" pin="D4" pad="35"/>
<connect gate="D" pin="D5" pad="37"/>
<connect gate="D" pin="D6" pad="38"/>
<connect gate="D" pin="D7" pad="39"/>
<connect gate="D" pin="D8" pad="40"/>
<connect gate="D" pin="D9" pad="41"/>
<connect gate="P1" pin="GND" pad="2"/>
<connect gate="P10" pin="VDDIO" pad="62"/>
<connect gate="P11" pin="VDDIO" pad="81"/>
<connect gate="P12" pin="VDDCORE" pad="27"/>
<connect gate="P13" pin="VDDCORE" pad="61"/>
<connect gate="P14" pin="VDDCORE" pad="94"/>
<connect gate="P15" pin="VDDIO" pad="10"/>
<connect gate="P16" pin="VDDIO" pad="28"/>
<connect gate="P17" pin="VDDIO" pad="44"/>
<connect gate="P18" pin="VDDIO" pad="95"/>
<connect gate="P2" pin="GND" pad="18"/>
<connect gate="P3" pin="GND" pad="19"/>
<connect gate="P4" pin="GND" pad="36"/>
<connect gate="P5" pin="GND" pad="52"/>
<connect gate="P6" pin="GND" pad="53"/>
<connect gate="P7" pin="GND" pad="65"/>
<connect gate="P8" pin="GND" pad="86"/>
<connect gate="P9" pin="GND" pad="87"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY26*" prefix="IC">
<description>&lt;b&gt;8-bit AVR Microcontroller with 2K Bytes Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com .. doc1477.pdf</description>
<gates>
<gate name="G$1" symbol="TINY26"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="20"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="19"/>
<connect gate="G$1" pin="(ADC10/!RESET!)PB7" pad="10"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="18"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="14"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="13"/>
<connect gate="G$1" pin="(ADC5/AIN0)PA6" pad="12"/>
<connect gate="G$1" pin="(ADC6/AIN1)PA7" pad="11"/>
<connect gate="G$1" pin="(ADC7/XTAL1)PB4" pad="7"/>
<connect gate="G$1" pin="(ADC8/XTAL2)PB5" pad="8"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="9"/>
<connect gate="G$1" pin="(AREF)PA3" pad="17"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="2"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/!OC1A!)PB0" pad="1"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="4"/>
<connect gate="G$1" pin="(SCK/SCL/!OC1B!)PB2" pad="3"/>
<connect gate="G$1" pin="AVCC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY261-20PU"/>
<attribute name="OC_FARNELL" value="1455146"/>
<attribute name="OC_NEWARK" value="58M3782"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY26L-8PU"/>
<attribute name="OC_FARNELL" value="9171657"/>
<attribute name="OC_NEWARK" value="01M6920"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="20"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="19"/>
<connect gate="G$1" pin="(ADC10/!RESET!)PB7" pad="10"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="18"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="14"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="13"/>
<connect gate="G$1" pin="(ADC5/AIN0)PA6" pad="12"/>
<connect gate="G$1" pin="(ADC6/AIN1)PA7" pad="11"/>
<connect gate="G$1" pin="(ADC7/XTAL1)PB4" pad="7"/>
<connect gate="G$1" pin="(ADC8/XTAL2)PB5" pad="8"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="9"/>
<connect gate="G$1" pin="(AREF)PA3" pad="17"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="2"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/!OC1A!)PB0" pad="1"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="4"/>
<connect gate="G$1" pin="(SCK/SCL/!OC1B!)PB2" pad="3"/>
<connect gate="G$1" pin="AVCC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY261-20SU"/>
<attribute name="OC_FARNELL" value="1455147"/>
<attribute name="OC_NEWARK" value="58M3783"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY26L-8SU"/>
<attribute name="OC_FARNELL" value="9171665"/>
<attribute name="OC_NEWARK" value="01M6921"/>
</technology>
</technologies>
</device>
<device name="M" package="MLF32">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="26"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="25"/>
<connect gate="G$1" pin="(ADC10/!RESET!)PB7" pad="11"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="23"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="17"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="15"/>
<connect gate="G$1" pin="(ADC5/AIN0)PA6" pad="14"/>
<connect gate="G$1" pin="(ADC6/AIN1)PA7" pad="13"/>
<connect gate="G$1" pin="(ADC7/XTAL1)PB4" pad="7"/>
<connect gate="G$1" pin="(ADC8/XTAL2)PB5" pad="8"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="10"/>
<connect gate="G$1" pin="(AREF)PA3" pad="22"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="31"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/!OC1A!)PB0" pad="30"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="2"/>
<connect gate="G$1" pin="(SCK/SCL/!OC1B!)PB2" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="21"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAM9708" prefix="SAM9708">
<description>&lt;b&gt;128-voice Integrated Sound Synthesizer&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SAM9708"/>
<gate name="C" symbol="SAM9708-SND"/>
<gate name="B" symbol="D0-15"/>
<gate name="D" symbol="WA27"/>
<gate name="E" symbol="WD15"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="V1" symbol="VCC1"/>
<gate name="V2" symbol="VCC1"/>
<gate name="V3" symbol="VCC1"/>
<gate name="V4" symbol="VCC1"/>
<gate name="V5" symbol="VCC1"/>
<gate name="V6" symbol="VCC2"/>
<gate name="V7" symbol="VCC2"/>
<gate name="V8" symbol="VCC2"/>
<gate name="V9" symbol="VCC2"/>
<gate name="V10" symbol="VCC2"/>
<gate name="V11" symbol="VC3"/>
<gate name="V12" symbol="VC3"/>
<gate name="V13" symbol="VC3"/>
<gate name="V14" symbol="VC3"/>
<gate name="V15" symbol="VC3"/>
<gate name="V16" symbol="VC3"/>
<gate name="V17" symbol="VC3"/>
<gate name="V18" symbol="VC3"/>
</gates>
<devices>
<device name="" package="TQFP144">
<connects>
<connect gate="A" pin="!CAS" pad="104"/>
<connect gate="A" pin="!CS" pad="16"/>
<connect gate="A" pin="!IO16" pad="4"/>
<connect gate="A" pin="!PWDN" pad="137"/>
<connect gate="A" pin="!RAS" pad="103"/>
<connect gate="A" pin="!RD" pad="10"/>
<connect gate="A" pin="!REFRESH" pad="105"/>
<connect gate="A" pin="!RESET" pad="134"/>
<connect gate="A" pin="!WR" pad="11"/>
<connect gate="A" pin="A0" pad="12"/>
<connect gate="A" pin="A1" pad="13"/>
<connect gate="A" pin="A2" pad="15"/>
<connect gate="A" pin="CK_OUT" pad="91"/>
<connect gate="A" pin="IRQ" pad="14"/>
<connect gate="A" pin="LDTEST" pad="136"/>
<connect gate="A" pin="OVCK-OUT" pad="47"/>
<connect gate="A" pin="RBS" pad="92"/>
<connect gate="A" pin="READY" pad="7"/>
<connect gate="A" pin="TEST" pad="135"/>
<connect gate="A" pin="X1" pad="61"/>
<connect gate="A" pin="X2" pad="62"/>
<connect gate="B" pin="D0" pad="19"/>
<connect gate="B" pin="D1" pad="22"/>
<connect gate="B" pin="D10" pad="1"/>
<connect gate="B" pin="D11" pad="144"/>
<connect gate="B" pin="D12" pad="141"/>
<connect gate="B" pin="D13" pad="140"/>
<connect gate="B" pin="D14" pad="139"/>
<connect gate="B" pin="D15" pad="138"/>
<connect gate="B" pin="D2" pad="23"/>
<connect gate="B" pin="D3" pad="24"/>
<connect gate="B" pin="D4" pad="25"/>
<connect gate="B" pin="D5" pad="26"/>
<connect gate="B" pin="D6" pad="27"/>
<connect gate="B" pin="D7" pad="28"/>
<connect gate="B" pin="D8" pad="3"/>
<connect gate="B" pin="D9" pad="2"/>
<connect gate="C" pin="!WCS0" pad="89"/>
<connect gate="C" pin="!WCS1" pad="90"/>
<connect gate="C" pin="!WOE" pad="88"/>
<connect gate="C" pin="!WWE" pad="87"/>
<connect gate="C" pin="BCK-OUT" pad="46"/>
<connect gate="C" pin="LFT" pad="60"/>
<connect gate="C" pin="MIDI1_IN" pad="29"/>
<connect gate="C" pin="MIDI1_OUT" pad="31"/>
<connect gate="C" pin="MIDI2_IN" pad="30"/>
<connect gate="C" pin="MIDI2_OUT" pad="32"/>
<connect gate="C" pin="SD-IN0" pad="33"/>
<connect gate="C" pin="SD-IN1" pad="34"/>
<connect gate="C" pin="SD-IN2" pad="37"/>
<connect gate="C" pin="SD-IN3" pad="38"/>
<connect gate="C" pin="SD-IN4" pad="48"/>
<connect gate="C" pin="SD-IN5" pad="49"/>
<connect gate="C" pin="SD-IN6" pad="50"/>
<connect gate="C" pin="SD-IN7" pad="53"/>
<connect gate="C" pin="SD-OUT0" pad="39"/>
<connect gate="C" pin="SD-OUT1" pad="40"/>
<connect gate="C" pin="SD-OUT2" pad="43"/>
<connect gate="C" pin="SD-OUT3" pad="44"/>
<connect gate="C" pin="SD-OUT4" pad="54"/>
<connect gate="C" pin="SD-OUT5" pad="55"/>
<connect gate="C" pin="SD-OUT6" pad="56"/>
<connect gate="C" pin="SD-OUT7" pad="57"/>
<connect gate="C" pin="WS-OUT" pad="45"/>
<connect gate="D" pin="WA0" pad="93"/>
<connect gate="D" pin="WA1" pad="94"/>
<connect gate="D" pin="WA10" pad="114"/>
<connect gate="D" pin="WA11" pad="115"/>
<connect gate="D" pin="WA12" pad="116"/>
<connect gate="D" pin="WA13" pad="117"/>
<connect gate="D" pin="WA14" pad="118"/>
<connect gate="D" pin="WA15" pad="119"/>
<connect gate="D" pin="WA16" pad="120"/>
<connect gate="D" pin="WA17" pad="121"/>
<connect gate="D" pin="WA18" pad="122"/>
<connect gate="D" pin="WA19" pad="123"/>
<connect gate="D" pin="WA2" pad="95"/>
<connect gate="D" pin="WA20" pad="126"/>
<connect gate="D" pin="WA21" pad="127"/>
<connect gate="D" pin="WA22" pad="128"/>
<connect gate="D" pin="WA23" pad="129"/>
<connect gate="D" pin="WA24" pad="130"/>
<connect gate="D" pin="WA25" pad="131"/>
<connect gate="D" pin="WA26" pad="132"/>
<connect gate="D" pin="WA3" pad="96"/>
<connect gate="D" pin="WA4" pad="101"/>
<connect gate="D" pin="WA5" pad="102"/>
<connect gate="D" pin="WA6" pad="106"/>
<connect gate="D" pin="WA7" pad="107"/>
<connect gate="D" pin="WA8" pad="108"/>
<connect gate="D" pin="WA9" pad="111"/>
<connect gate="E" pin="WD0" pad="86"/>
<connect gate="E" pin="WD1" pad="85"/>
<connect gate="E" pin="WD10" pad="72"/>
<connect gate="E" pin="WD11" pad="71"/>
<connect gate="E" pin="WD12" pad="68"/>
<connect gate="E" pin="WD13" pad="67"/>
<connect gate="E" pin="WD14" pad="66"/>
<connect gate="E" pin="WD15" pad="65"/>
<connect gate="E" pin="WD2" pad="84"/>
<connect gate="E" pin="WD3" pad="79"/>
<connect gate="E" pin="WD4" pad="78"/>
<connect gate="E" pin="WD5" pad="77"/>
<connect gate="E" pin="WD6" pad="76"/>
<connect gate="E" pin="WD7" pad="75"/>
<connect gate="E" pin="WD8" pad="74"/>
<connect gate="E" pin="WD9" pad="73"/>
<connect gate="G1" pin="GND" pad="6"/>
<connect gate="G10" pin="GND" pad="70"/>
<connect gate="G11" pin="GND" pad="82"/>
<connect gate="G12" pin="GND" pad="83"/>
<connect gate="G13" pin="GND" pad="98"/>
<connect gate="G14" pin="GND" pad="100"/>
<connect gate="G15" pin="GND" pad="110"/>
<connect gate="G16" pin="GND" pad="113"/>
<connect gate="G17" pin="GND" pad="125"/>
<connect gate="G18" pin="GND" pad="133"/>
<connect gate="G19" pin="GND" pad="143"/>
<connect gate="G2" pin="GND" pad="9"/>
<connect gate="G3" pin="GND" pad="18"/>
<connect gate="G4" pin="GND" pad="21"/>
<connect gate="G5" pin="GND" pad="36"/>
<connect gate="G6" pin="GND" pad="42"/>
<connect gate="G7" pin="GND" pad="51"/>
<connect gate="G8" pin="GND" pad="59"/>
<connect gate="G9" pin="GND" pad="64"/>
<connect gate="V1" pin="VCC1" pad="5"/>
<connect gate="V10" pin="VCC2" pad="124"/>
<connect gate="V11" pin="VC3" pad="8"/>
<connect gate="V12" pin="VC3" pad="17"/>
<connect gate="V13" pin="VC3" pad="41"/>
<connect gate="V14" pin="VC3" pad="58"/>
<connect gate="V15" pin="VC3" pad="63"/>
<connect gate="V16" pin="VC3" pad="80"/>
<connect gate="V17" pin="VC3" pad="99"/>
<connect gate="V18" pin="VC3" pad="112"/>
<connect gate="V2" pin="VCC1" pad="20"/>
<connect gate="V3" pin="VCC1" pad="35"/>
<connect gate="V4" pin="VCC1" pad="52"/>
<connect gate="V5" pin="VCC1" pad="142"/>
<connect gate="V6" pin="VCC2" pad="69"/>
<connect gate="V7" pin="VCC2" pad="81"/>
<connect gate="V8" pin="VCC2" pad="97"/>
<connect gate="V9" pin="VCC2" pad="109"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T8*C5121" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with Multiprotocol Smart Card Interface&lt;/b&gt;&lt;p&gt;
Source: Uploaded by Heiko Künzel &lt;heiko.kuenzel@atg-gera.de&gt; from ATG Automatisierungstechnik Gera&lt;br&gt;
Mon Mar 10 13:32:48 2003 Atmel-Library mit zusätzlich T83C5121-Prozessor im SSOP24-Package.</description>
<gates>
<gate name="G$1" symbol="T8XC5121"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="CVCC" pad="3"/>
<connect gate="G$1" pin="CVSS" pad="1"/>
<connect gate="G$1" pin="DVCC" pad="22"/>
<connect gate="G$1" pin="EVCC" pad="23"/>
<connect gate="G$1" pin="LI" pad="2"/>
<connect gate="G$1" pin="P1.0/CIO" pad="9"/>
<connect gate="G$1" pin="P1.1/CC8" pad="8"/>
<connect gate="G$1" pin="P1.2/CPRES" pad="7"/>
<connect gate="G$1" pin="P1.3/CC4" pad="6"/>
<connect gate="G$1" pin="P1.4/CCLK" pad="5"/>
<connect gate="G$1" pin="P1.5/CRST" pad="4"/>
<connect gate="G$1" pin="P3.0/RXD" pad="20"/>
<connect gate="G$1" pin="P3.1/TXD" pad="19"/>
<connect gate="G$1" pin="P3.2/INT0" pad="16"/>
<connect gate="G$1" pin="P3.3/INT1" pad="18"/>
<connect gate="G$1" pin="P3.4/T0" pad="17"/>
<connect gate="G$1" pin="P3.5/CIO1" pad="15"/>
<connect gate="G$1" pin="P3.6/CCLK1/LED0" pad="14"/>
<connect gate="G$1" pin="P3.7/CRST1/LED1" pad="13"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="VCC" pad="24"/>
<connect gate="G$1" pin="VSS" pad="21"/>
<connect gate="G$1" pin="XTAL1" pad="12"/>
<connect gate="G$1" pin="XTAL2" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T8?C5121" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with Multiprotocol Smart Card Interface&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/...doc4164.pdf</description>
<gates>
<gate name="G$1" symbol="T8X5121-PLCC52"/>
</gates>
<devices>
<device name="3" package="PLCC52">
<connects>
<connect gate="G$1" pin="!RST" pad="20"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="CVCC" pad="6"/>
<connect gate="G$1" pin="CVSS" pad="2"/>
<connect gate="G$1" pin="DVCC" pad="46"/>
<connect gate="G$1" pin="EA" pad="10"/>
<connect gate="G$1" pin="EVCC" pad="51"/>
<connect gate="G$1" pin="LI" pad="3"/>
<connect gate="G$1" pin="P0.0/AD0" pad="42"/>
<connect gate="G$1" pin="P0.1/AD1" pad="41"/>
<connect gate="G$1" pin="P0.2/AD2" pad="40"/>
<connect gate="G$1" pin="P0.3/AD3" pad="39"/>
<connect gate="G$1" pin="P0.4/AD4" pad="33"/>
<connect gate="G$1" pin="P0.5/AD5" pad="21"/>
<connect gate="G$1" pin="P0.6/AD6" pad="38"/>
<connect gate="G$1" pin="P0.7/AD7" pad="30"/>
<connect gate="G$1" pin="P1.0/CIO" pad="18"/>
<connect gate="G$1" pin="P1.1/CC8" pad="17"/>
<connect gate="G$1" pin="P1.2/CPRES" pad="16"/>
<connect gate="G$1" pin="P1.3/CC4" pad="9"/>
<connect gate="G$1" pin="P1.4/CCLK" pad="8"/>
<connect gate="G$1" pin="P1.5/CRST" pad="7"/>
<connect gate="G$1" pin="P2.0/A8" pad="29"/>
<connect gate="G$1" pin="P2.1/A9" pad="28"/>
<connect gate="G$1" pin="P2.2/A10" pad="27"/>
<connect gate="G$1" pin="P2.3/A11" pad="26"/>
<connect gate="G$1" pin="P2.4/A12" pad="19"/>
<connect gate="G$1" pin="P2.5/A13" pad="15"/>
<connect gate="G$1" pin="P2.6/A14" pad="14"/>
<connect gate="G$1" pin="P2.7/A15" pad="13"/>
<connect gate="G$1" pin="P3.0/RXD" pad="44"/>
<connect gate="G$1" pin="P3.1/TXD" pad="43"/>
<connect gate="G$1" pin="P3.2/INT0" pad="35"/>
<connect gate="G$1" pin="P3.3/INT1" pad="37"/>
<connect gate="G$1" pin="P3.4/T0" pad="36"/>
<connect gate="G$1" pin="P3.5/CIO1" pad="34"/>
<connect gate="G$1" pin="P3.6/CCLK1/LED0" pad="32"/>
<connect gate="G$1" pin="P3.7/CRST1/LED1" pad="31"/>
<connect gate="G$1" pin="PSEN" pad="11"/>
<connect gate="G$1" pin="VCC" pad="24"/>
<connect gate="G$1" pin="VCC@1" pad="1"/>
<connect gate="G$1" pin="VSS" pad="25"/>
<connect gate="G$1" pin="VSS@1" pad="45"/>
<connect gate="G$1" pin="XTAL1" pad="23"/>
<connect gate="G$1" pin="XTAL2" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5" package="PLCC52">
<connects>
<connect gate="G$1" pin="!RST" pad="20"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="CVCC" pad="6"/>
<connect gate="G$1" pin="CVSS" pad="2"/>
<connect gate="G$1" pin="DVCC" pad="46"/>
<connect gate="G$1" pin="EA" pad="10"/>
<connect gate="G$1" pin="EVCC" pad="51"/>
<connect gate="G$1" pin="LI" pad="3"/>
<connect gate="G$1" pin="P0.0/AD0" pad="42"/>
<connect gate="G$1" pin="P0.1/AD1" pad="41"/>
<connect gate="G$1" pin="P0.2/AD2" pad="40"/>
<connect gate="G$1" pin="P0.3/AD3" pad="39"/>
<connect gate="G$1" pin="P0.4/AD4" pad="33"/>
<connect gate="G$1" pin="P0.5/AD5" pad="21"/>
<connect gate="G$1" pin="P0.6/AD6" pad="38"/>
<connect gate="G$1" pin="P0.7/AD7" pad="30"/>
<connect gate="G$1" pin="P1.0/CIO" pad="18"/>
<connect gate="G$1" pin="P1.1/CC8" pad="17"/>
<connect gate="G$1" pin="P1.2/CPRES" pad="16"/>
<connect gate="G$1" pin="P1.3/CC4" pad="9"/>
<connect gate="G$1" pin="P1.4/CCLK" pad="8"/>
<connect gate="G$1" pin="P1.5/CRST" pad="7"/>
<connect gate="G$1" pin="P2.0/A8" pad="29"/>
<connect gate="G$1" pin="P2.1/A9" pad="28"/>
<connect gate="G$1" pin="P2.2/A10" pad="27"/>
<connect gate="G$1" pin="P2.3/A11" pad="26"/>
<connect gate="G$1" pin="P2.4/A12" pad="19"/>
<connect gate="G$1" pin="P2.5/A13" pad="15"/>
<connect gate="G$1" pin="P2.6/A14" pad="14"/>
<connect gate="G$1" pin="P2.7/A15" pad="13"/>
<connect gate="G$1" pin="P3.0/RXD" pad="44"/>
<connect gate="G$1" pin="P3.1/TXD" pad="43"/>
<connect gate="G$1" pin="P3.2/INT0" pad="35"/>
<connect gate="G$1" pin="P3.3/INT1" pad="37"/>
<connect gate="G$1" pin="P3.4/T0" pad="36"/>
<connect gate="G$1" pin="P3.5/CIO1" pad="34"/>
<connect gate="G$1" pin="P3.6/CCLK1/LED0" pad="32"/>
<connect gate="G$1" pin="P3.7/CRST1/LED1" pad="31"/>
<connect gate="G$1" pin="PSEN" pad="11"/>
<connect gate="G$1" pin="VCC" pad="24"/>
<connect gate="G$1" pin="VCC@1" pad="1"/>
<connect gate="G$1" pin="VSS" pad="25"/>
<connect gate="G$1" pin="VSS@1" pad="45"/>
<connect gate="G$1" pin="XTAL1" pad="23"/>
<connect gate="G$1" pin="XTAL2" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="9" package="PLCC52">
<connects>
<connect gate="G$1" pin="!RST" pad="20"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="CVCC" pad="6"/>
<connect gate="G$1" pin="CVSS" pad="2"/>
<connect gate="G$1" pin="DVCC" pad="46"/>
<connect gate="G$1" pin="EA" pad="10"/>
<connect gate="G$1" pin="EVCC" pad="51"/>
<connect gate="G$1" pin="LI" pad="3"/>
<connect gate="G$1" pin="P0.0/AD0" pad="42"/>
<connect gate="G$1" pin="P0.1/AD1" pad="41"/>
<connect gate="G$1" pin="P0.2/AD2" pad="40"/>
<connect gate="G$1" pin="P0.3/AD3" pad="39"/>
<connect gate="G$1" pin="P0.4/AD4" pad="33"/>
<connect gate="G$1" pin="P0.5/AD5" pad="21"/>
<connect gate="G$1" pin="P0.6/AD6" pad="38"/>
<connect gate="G$1" pin="P0.7/AD7" pad="30"/>
<connect gate="G$1" pin="P1.0/CIO" pad="18"/>
<connect gate="G$1" pin="P1.1/CC8" pad="17"/>
<connect gate="G$1" pin="P1.2/CPRES" pad="16"/>
<connect gate="G$1" pin="P1.3/CC4" pad="9"/>
<connect gate="G$1" pin="P1.4/CCLK" pad="8"/>
<connect gate="G$1" pin="P1.5/CRST" pad="7"/>
<connect gate="G$1" pin="P2.0/A8" pad="29"/>
<connect gate="G$1" pin="P2.1/A9" pad="28"/>
<connect gate="G$1" pin="P2.2/A10" pad="27"/>
<connect gate="G$1" pin="P2.3/A11" pad="26"/>
<connect gate="G$1" pin="P2.4/A12" pad="19"/>
<connect gate="G$1" pin="P2.5/A13" pad="15"/>
<connect gate="G$1" pin="P2.6/A14" pad="14"/>
<connect gate="G$1" pin="P2.7/A15" pad="13"/>
<connect gate="G$1" pin="P3.0/RXD" pad="44"/>
<connect gate="G$1" pin="P3.1/TXD" pad="43"/>
<connect gate="G$1" pin="P3.2/INT0" pad="35"/>
<connect gate="G$1" pin="P3.3/INT1" pad="37"/>
<connect gate="G$1" pin="P3.4/T0" pad="36"/>
<connect gate="G$1" pin="P3.5/CIO1" pad="34"/>
<connect gate="G$1" pin="P3.6/CCLK1/LED0" pad="32"/>
<connect gate="G$1" pin="P3.7/CRST1/LED1" pad="31"/>
<connect gate="G$1" pin="PSEN" pad="11"/>
<connect gate="G$1" pin="VCC" pad="24"/>
<connect gate="G$1" pin="VCC@1" pad="1"/>
<connect gate="G$1" pin="VSS" pad="25"/>
<connect gate="G$1" pin="VSS@1" pad="45"/>
<connect gate="G$1" pin="XTAL1" pad="23"/>
<connect gate="G$1" pin="XTAL2" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT8*C51SND1C" prefix="IC">
<description>&lt;b&gt;Single-Chip Flash Microcontroller&lt;/b&gt;&lt;p&gt;
with MP3 Decoder and Human Interface&lt;br&gt;
Source: www.atmel.com .. doc4109.pdf</description>
<gates>
<gate name="G$1" symbol="AT89C51SND1C"/>
<gate name="P" symbol="P-AT89C51SND1C"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="G$1" pin="!ISP" pad="13"/>
<connect gate="G$1" pin="!TST" pad="30"/>
<connect gate="G$1" pin="AIN0" pad="49"/>
<connect gate="G$1" pin="AIN1" pad="50"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="AREFN" pad="48"/>
<connect gate="G$1" pin="AREFP" pad="47"/>
<connect gate="G$1" pin="AVDD" pad="45"/>
<connect gate="G$1" pin="AVSS" pad="46"/>
<connect gate="G$1" pin="D+" pad="33"/>
<connect gate="G$1" pin="D-" pad="34"/>
<connect gate="G$1" pin="DCLK" pad="57"/>
<connect gate="G$1" pin="DESL" pad="58"/>
<connect gate="G$1" pin="DOUT" pad="56"/>
<connect gate="G$1" pin="FILT" pad="24"/>
<connect gate="G$1" pin="MCLK" pad="63"/>
<connect gate="G$1" pin="MCMD" pad="61"/>
<connect gate="G$1" pin="MDAT" pad="62"/>
<connect gate="G$1" pin="P0.0/AD0" pad="8"/>
<connect gate="G$1" pin="P0.1/AD1" pad="7"/>
<connect gate="G$1" pin="P0.2/AD2" pad="6"/>
<connect gate="G$1" pin="P0.3/AD3" pad="5"/>
<connect gate="G$1" pin="P0.4/AD4" pad="4"/>
<connect gate="G$1" pin="P0.5/AD5" pad="3"/>
<connect gate="G$1" pin="P0.6/AD6" pad="84"/>
<connect gate="G$1" pin="P0.7/AD7" pad="83"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="14"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="15"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="16"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="17"/>
<connect gate="G$1" pin="P1.4" pad="18"/>
<connect gate="G$1" pin="P1.5" pad="19"/>
<connect gate="G$1" pin="P1.6/SCL" pad="20"/>
<connect gate="G$1" pin="P1.7/SDA" pad="21"/>
<connect gate="G$1" pin="P2.0/A8" pad="78"/>
<connect gate="G$1" pin="P2.1/A9" pad="77"/>
<connect gate="G$1" pin="P2.2/A10" pad="71"/>
<connect gate="G$1" pin="P2.3/A11" pad="70"/>
<connect gate="G$1" pin="P2.4/A12" pad="69"/>
<connect gate="G$1" pin="P2.5/A13" pad="68"/>
<connect gate="G$1" pin="P2.6/A14" pad="67"/>
<connect gate="G$1" pin="P2.7/A15" pad="66"/>
<connect gate="G$1" pin="P3.0/RXD" pad="37"/>
<connect gate="G$1" pin="P3.1/TXD" pad="38"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="39"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="40"/>
<connect gate="G$1" pin="P3.4/T0" pad="41"/>
<connect gate="G$1" pin="P3.5/T1" pad="42"/>
<connect gate="G$1" pin="P3.6/!WR" pad="43"/>
<connect gate="G$1" pin="P3.7/!RD" pad="44"/>
<connect gate="G$1" pin="P4.0/MISO" pad="79"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="80"/>
<connect gate="G$1" pin="P4.2/SCK" pad="81"/>
<connect gate="G$1" pin="P4.3/!SS" pad="82"/>
<connect gate="G$1" pin="P4.4" pad="72"/>
<connect gate="G$1" pin="P4.5" pad="73"/>
<connect gate="G$1" pin="P4.6" pad="75"/>
<connect gate="G$1" pin="P4.7" pad="76"/>
<connect gate="G$1" pin="P5.0" pad="9"/>
<connect gate="G$1" pin="P5.1" pad="10"/>
<connect gate="G$1" pin="P5.2" pad="51"/>
<connect gate="G$1" pin="P5.3" pad="52"/>
<connect gate="G$1" pin="RST" pad="60"/>
<connect gate="G$1" pin="SCLK" pad="59"/>
<connect gate="G$1" pin="X1" pad="29"/>
<connect gate="G$1" pin="X2" pad="27"/>
<connect gate="P" pin="PVDD" pad="23"/>
<connect gate="P" pin="PVSS" pad="25"/>
<connect gate="P" pin="UVDD" pad="31"/>
<connect gate="P" pin="UVSS" pad="32"/>
<connect gate="P" pin="VDD@1" pad="1"/>
<connect gate="P" pin="VDD@2" pad="22"/>
<connect gate="P" pin="VDD@3" pad="35"/>
<connect gate="P" pin="VDD@4" pad="54"/>
<connect gate="P" pin="VDD@5" pad="64"/>
<connect gate="P" pin="VSS@1" pad="2"/>
<connect gate="P" pin="VSS@2" pad="26"/>
<connect gate="P" pin="VSS@3" pad="36"/>
<connect gate="P" pin="VSS@4" pad="55"/>
<connect gate="P" pin="VSS@5" pad="65"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1095728"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-RO" package="TQFP80">
<connects>
<connect gate="G$1" pin="!ISP" pad="2"/>
<connect gate="G$1" pin="!TST" pad="18"/>
<connect gate="G$1" pin="AIN0" pad="37"/>
<connect gate="G$1" pin="AIN1" pad="38"/>
<connect gate="G$1" pin="ALE" pad="1"/>
<connect gate="G$1" pin="AREFN" pad="36"/>
<connect gate="G$1" pin="AREFP" pad="35"/>
<connect gate="G$1" pin="AVDD" pad="33"/>
<connect gate="G$1" pin="AVSS" pad="34"/>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="22"/>
<connect gate="G$1" pin="DCLK" pad="44"/>
<connect gate="G$1" pin="DESL" pad="45"/>
<connect gate="G$1" pin="DOUT" pad="43"/>
<connect gate="G$1" pin="FILT" pad="13"/>
<connect gate="G$1" pin="MCLK" pad="50"/>
<connect gate="G$1" pin="MCMD" pad="48"/>
<connect gate="G$1" pin="MDAT" pad="49"/>
<connect gate="G$1" pin="P0.0/AD0" pad="78"/>
<connect gate="G$1" pin="P0.1/AD1" pad="77"/>
<connect gate="G$1" pin="P0.2/AD2" pad="76"/>
<connect gate="G$1" pin="P0.3/AD3" pad="75"/>
<connect gate="G$1" pin="P0.4/AD4" pad="74"/>
<connect gate="G$1" pin="P0.5/AD5" pad="73"/>
<connect gate="G$1" pin="P0.6/AD6" pad="70"/>
<connect gate="G$1" pin="P0.7/AD7" pad="69"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="3"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="4"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="5"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="6"/>
<connect gate="G$1" pin="P1.4" pad="7"/>
<connect gate="G$1" pin="P1.5" pad="8"/>
<connect gate="G$1" pin="P1.6/SCL" pad="9"/>
<connect gate="G$1" pin="P1.7/SDA" pad="10"/>
<connect gate="G$1" pin="P2.0/A8" pad="64"/>
<connect gate="G$1" pin="P2.1/A9" pad="63"/>
<connect gate="G$1" pin="P2.2/A10" pad="58"/>
<connect gate="G$1" pin="P2.3/A11" pad="57"/>
<connect gate="G$1" pin="P2.4/A12" pad="56"/>
<connect gate="G$1" pin="P2.5/A13" pad="55"/>
<connect gate="G$1" pin="P2.6/A14" pad="54"/>
<connect gate="G$1" pin="P2.7/A15" pad="53"/>
<connect gate="G$1" pin="P3.0/RXD" pad="25"/>
<connect gate="G$1" pin="P3.1/TXD" pad="26"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="27"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="28"/>
<connect gate="G$1" pin="P3.4/T0" pad="29"/>
<connect gate="G$1" pin="P3.5/T1" pad="30"/>
<connect gate="G$1" pin="P3.6/!WR" pad="31"/>
<connect gate="G$1" pin="P3.7/!RD" pad="32"/>
<connect gate="G$1" pin="P4.0/MISO" pad="65"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="66"/>
<connect gate="G$1" pin="P4.2/SCK" pad="67"/>
<connect gate="G$1" pin="P4.3/!SS" pad="68"/>
<connect gate="G$1" pin="P4.4" pad="59"/>
<connect gate="G$1" pin="P4.5" pad="60"/>
<connect gate="G$1" pin="P4.6" pad="61"/>
<connect gate="G$1" pin="P4.7" pad="62"/>
<connect gate="G$1" pin="P5.0" pad="79"/>
<connect gate="G$1" pin="P5.1" pad="80"/>
<connect gate="G$1" pin="P5.2" pad="39"/>
<connect gate="G$1" pin="P5.3" pad="40"/>
<connect gate="G$1" pin="RST" pad="47"/>
<connect gate="G$1" pin="SCLK" pad="46"/>
<connect gate="G$1" pin="X1" pad="17"/>
<connect gate="G$1" pin="X2" pad="16"/>
<connect gate="P" pin="PVDD" pad="51"/>
<connect gate="P" pin="PVSS" pad="14"/>
<connect gate="P" pin="UVDD" pad="19"/>
<connect gate="P" pin="UVSS" pad="20"/>
<connect gate="P" pin="VDD@1" pad="11"/>
<connect gate="P" pin="VDD@2" pad="12"/>
<connect gate="P" pin="VDD@3" pad="23"/>
<connect gate="P" pin="VDD@4" pad="41"/>
<connect gate="P" pin="VDD@5" pad="71"/>
<connect gate="P" pin="VSS@1" pad="15"/>
<connect gate="P" pin="VSS@2" pad="24"/>
<connect gate="P" pin="VSS@3" pad="42"/>
<connect gate="P" pin="VSS@4" pad="52"/>
<connect gate="P" pin="VSS@5" pad="72"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1095728"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-7H" package="BGA81">
<connects>
<connect gate="G$1" pin="!ISP" pad="B2"/>
<connect gate="G$1" pin="!TST" pad="G2"/>
<connect gate="G$1" pin="AIN0" pad="H5"/>
<connect gate="G$1" pin="AIN1" pad="H7"/>
<connect gate="G$1" pin="ALE" pad="A1"/>
<connect gate="G$1" pin="AREFN" pad="J6"/>
<connect gate="G$1" pin="AREFP" pad="J7"/>
<connect gate="G$1" pin="AVDD" pad="F5"/>
<connect gate="G$1" pin="AVSS" pad="H6"/>
<connect gate="G$1" pin="D+" pad="J1"/>
<connect gate="G$1" pin="D-" pad="H2"/>
<connect gate="G$1" pin="DCLK" pad="H9"/>
<connect gate="G$1" pin="DESL" pad="G9"/>
<connect gate="G$1" pin="DOUT" pad="G7"/>
<connect gate="G$1" pin="FILT" pad="E4"/>
<connect gate="G$1" pin="MCLK" pad="F7"/>
<connect gate="G$1" pin="MCMD" pad="F8"/>
<connect gate="G$1" pin="MDAT" pad="F6"/>
<connect gate="G$1" pin="P0.0/AD0" pad="B3"/>
<connect gate="G$1" pin="P0.1/AD1" pad="B5"/>
<connect gate="G$1" pin="P0.2/AD2" pad="A4"/>
<connect gate="G$1" pin="P0.3/AD3" pad="A3"/>
<connect gate="G$1" pin="P0.4/AD4" pad="B4"/>
<connect gate="G$1" pin="P0.5/AD5" pad="D5"/>
<connect gate="G$1" pin="P0.6/AD6" pad="C6"/>
<connect gate="G$1" pin="P0.7/AD7" pad="D6"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="C3"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="B1"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="C1"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="C2"/>
<connect gate="G$1" pin="P1.4" pad="D1"/>
<connect gate="G$1" pin="P1.5" pad="D2"/>
<connect gate="G$1" pin="P1.6/SCL" pad="D4"/>
<connect gate="G$1" pin="P1.7/SDA" pad="D3"/>
<connect gate="G$1" pin="P2.0/A8" pad="A8"/>
<connect gate="G$1" pin="P2.1/A9" pad="C7"/>
<connect gate="G$1" pin="P2.2/A10" pad="C8"/>
<connect gate="G$1" pin="P2.3/A11" pad="E8"/>
<connect gate="G$1" pin="P2.4/A12" pad="D9"/>
<connect gate="G$1" pin="P2.5/A13" pad="C9"/>
<connect gate="G$1" pin="P2.6/A14" pad="D8"/>
<connect gate="G$1" pin="P2.7/A15" pad="E6"/>
<connect gate="G$1" pin="P3.0/RXD" pad="J3"/>
<connect gate="G$1" pin="P3.1/TXD" pad="H3"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="J4"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="H4"/>
<connect gate="G$1" pin="P3.4/T0" pad="F4"/>
<connect gate="G$1" pin="P3.5/T1" pad="G4"/>
<connect gate="G$1" pin="P3.6/!WR" pad="J5"/>
<connect gate="G$1" pin="P3.7/!RD" pad="G5"/>
<connect gate="G$1" pin="P4.0/MISO" pad="A7"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="B7"/>
<connect gate="G$1" pin="P4.2/SCK" pad="A6"/>
<connect gate="G$1" pin="P4.3/!SS" pad="B6"/>
<connect gate="G$1" pin="P4.4" pad="B9"/>
<connect gate="G$1" pin="P4.5" pad="D7"/>
<connect gate="G$1" pin="P4.6" pad="A9"/>
<connect gate="G$1" pin="P4.7" pad="B8"/>
<connect gate="G$1" pin="P5.0" pad="A2"/>
<connect gate="G$1" pin="P5.1" pad="C4"/>
<connect gate="G$1" pin="P5.2" pad="J8"/>
<connect gate="G$1" pin="P5.3" pad="G6"/>
<connect gate="G$1" pin="RST" pad="F9"/>
<connect gate="G$1" pin="SCLK" pad="G8"/>
<connect gate="G$1" pin="X1" pad="E2"/>
<connect gate="G$1" pin="X2" pad="F1"/>
<connect gate="P" pin="PVDD" pad="E3"/>
<connect gate="P" pin="PVSS" pad="F2"/>
<connect gate="P" pin="UVDD" pad="H1"/>
<connect gate="P" pin="UVSS" pad="F3"/>
<connect gate="P" pin="VDD@1" pad="A5"/>
<connect gate="P" pin="VDD@2" pad="E1"/>
<connect gate="P" pin="VDD@3" pad="E9"/>
<connect gate="P" pin="VDD@4" pad="G3"/>
<connect gate="P" pin="VDD@5" pad="J9"/>
<connect gate="P" pin="VSS@1" pad="C5"/>
<connect gate="P" pin="VSS@2" pad="E7"/>
<connect gate="P" pin="VSS@3" pad="G1"/>
<connect gate="P" pin="VSS@4" pad="H8"/>
<connect gate="P" pin="VSS@5" pad="J2"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C51-*" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 4K Bytes Flash&lt;/b&gt;&lt;p&gt;
&lt;font color="red"&gt;Not Recommended for New Designs. Use AT89S51.&lt;/font&gt;&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc0265.</description>
<gates>
<gate name="G$1" symbol="AT89C51"/>
</gates>
<devices>
<device name="PC" package="DIL40">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="31"/>
<connect gate="G$1" pin="!PSEN" pad="29"/>
<connect gate="G$1" pin="ALE/!PROG" pad="30"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="P0.0_AD0" pad="39"/>
<connect gate="G$1" pin="P0.1_AD1" pad="38"/>
<connect gate="G$1" pin="P0.2_AD2" pad="37"/>
<connect gate="G$1" pin="P0.3_AD3" pad="36"/>
<connect gate="G$1" pin="P0.4_AD4" pad="35"/>
<connect gate="G$1" pin="P0.5_AD5" pad="34"/>
<connect gate="G$1" pin="P0.6_AD6" pad="33"/>
<connect gate="G$1" pin="P0.7_AD7" pad="32"/>
<connect gate="G$1" pin="P1.0" pad="1"/>
<connect gate="G$1" pin="P1.1" pad="2"/>
<connect gate="G$1" pin="P1.2" pad="3"/>
<connect gate="G$1" pin="P1.3" pad="4"/>
<connect gate="G$1" pin="P1.4" pad="5"/>
<connect gate="G$1" pin="P1.5" pad="6"/>
<connect gate="G$1" pin="P1.6" pad="7"/>
<connect gate="G$1" pin="P1.7" pad="8"/>
<connect gate="G$1" pin="P2.0_A8" pad="21"/>
<connect gate="G$1" pin="P2.1_A9" pad="22"/>
<connect gate="G$1" pin="P2.2_A10" pad="23"/>
<connect gate="G$1" pin="P2.3_A11" pad="24"/>
<connect gate="G$1" pin="P2.4_A12" pad="25"/>
<connect gate="G$1" pin="P2.5_A13" pad="26"/>
<connect gate="G$1" pin="P2.6_A14" pad="27"/>
<connect gate="G$1" pin="P2.7_A15" pad="28"/>
<connect gate="G$1" pin="P3.0/RXD" pad="10"/>
<connect gate="G$1" pin="P3.1/TXD" pad="11"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="12"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="13"/>
<connect gate="G$1" pin="P3.4/T0" pad="14"/>
<connect gate="G$1" pin="P3.5/T1" pad="15"/>
<connect gate="G$1" pin="P3.6/!WR" pad="16"/>
<connect gate="G$1" pin="P3.7/!RD" pad="17"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="16">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="20">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="JC" package="PLCC44">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="32"/>
<connect gate="G$1" pin="ALE/!PROG" pad="33"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="P0.0_AD0" pad="43"/>
<connect gate="G$1" pin="P0.1_AD1" pad="42"/>
<connect gate="G$1" pin="P0.2_AD2" pad="41"/>
<connect gate="G$1" pin="P0.3_AD3" pad="40"/>
<connect gate="G$1" pin="P0.4_AD4" pad="39"/>
<connect gate="G$1" pin="P0.5_AD5" pad="38"/>
<connect gate="G$1" pin="P0.6_AD6" pad="37"/>
<connect gate="G$1" pin="P0.7_AD7" pad="36"/>
<connect gate="G$1" pin="P1.0" pad="2"/>
<connect gate="G$1" pin="P1.1" pad="3"/>
<connect gate="G$1" pin="P1.2" pad="4"/>
<connect gate="G$1" pin="P1.3" pad="5"/>
<connect gate="G$1" pin="P1.4" pad="6"/>
<connect gate="G$1" pin="P1.5" pad="7"/>
<connect gate="G$1" pin="P1.6" pad="8"/>
<connect gate="G$1" pin="P1.7" pad="9"/>
<connect gate="G$1" pin="P2.0_A8" pad="24"/>
<connect gate="G$1" pin="P2.1_A9" pad="25"/>
<connect gate="G$1" pin="P2.2_A10" pad="26"/>
<connect gate="G$1" pin="P2.3_A11" pad="27"/>
<connect gate="G$1" pin="P2.4_A12" pad="28"/>
<connect gate="G$1" pin="P2.5_A13" pad="29"/>
<connect gate="G$1" pin="P2.6_A14" pad="30"/>
<connect gate="G$1" pin="P2.7_A15" pad="31"/>
<connect gate="G$1" pin="P3.0/RXD" pad="11"/>
<connect gate="G$1" pin="P3.1/TXD" pad="13"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="14"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="15"/>
<connect gate="G$1" pin="P3.4/T0" pad="16"/>
<connect gate="G$1" pin="P3.5/T1" pad="17"/>
<connect gate="G$1" pin="P3.6/!WR" pad="18"/>
<connect gate="G$1" pin="P3.7/!RD" pad="19"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51ED2-SLSUM"/>
<attribute name="OC_FARNELL" value="1095722"/>
<attribute name="OC_NEWARK" value="78K5790"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51ED2-SLSUM"/>
<attribute name="OC_FARNELL" value="1095722"/>
<attribute name="OC_NEWARK" value="78K5790"/>
</technology>
<technology name="16">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51RE2-SLSUM"/>
<attribute name="OC_FARNELL" value="1455062"/>
<attribute name="OC_NEWARK" value="58M3857"/>
</technology>
<technology name="20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51ED2-RLTUM"/>
<attribute name="OC_FARNELL" value="1095726"/>
<attribute name="OC_NEWARK" value="51P1802"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C51ED2-SLSUM"/>
<attribute name="OC_FARNELL" value="1095722"/>
<attribute name="OC_NEWARK" value="78K5790"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C51?*" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 4K Bytes Flash&lt;/b&gt;&lt;p&gt;
&lt;font color="red"&gt;Not Recommended for New Designs. Use AT89S51.&lt;/font&gt;&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc0265.</description>
<gates>
<gate name="G$1" symbol="AT89C51"/>
<gate name="P" symbol="GND"/>
</gates>
<devices>
<device name="AC" package="TQFP44">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE/!PROG" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="P0.0_AD0" pad="37"/>
<connect gate="G$1" pin="P0.1_AD1" pad="36"/>
<connect gate="G$1" pin="P0.2_AD2" pad="35"/>
<connect gate="G$1" pin="P0.3_AD3" pad="34"/>
<connect gate="G$1" pin="P0.4_AD4" pad="33"/>
<connect gate="G$1" pin="P0.5_AD5" pad="32"/>
<connect gate="G$1" pin="P0.6_AD6" pad="31"/>
<connect gate="G$1" pin="P0.7_AD7" pad="30"/>
<connect gate="G$1" pin="P1.0" pad="40"/>
<connect gate="G$1" pin="P1.1" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5" pad="1"/>
<connect gate="G$1" pin="P1.6" pad="2"/>
<connect gate="G$1" pin="P1.7" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0/RXD" pad="5"/>
<connect gate="G$1" pin="P3.1/TXD" pad="7"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="8"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/!WR" pad="12"/>
<connect gate="G$1" pin="P3.7/!RD" pad="13"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="17"/>
</connects>
<technologies>
<technology name="-12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-16">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="QC" package="PQFP44">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE/!PROG" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="P0.0_AD0" pad="37"/>
<connect gate="G$1" pin="P0.1_AD1" pad="36"/>
<connect gate="G$1" pin="P0.2_AD2" pad="35"/>
<connect gate="G$1" pin="P0.3_AD3" pad="34"/>
<connect gate="G$1" pin="P0.4_AD4" pad="33"/>
<connect gate="G$1" pin="P0.5_AD5" pad="32"/>
<connect gate="G$1" pin="P0.6_AD6" pad="31"/>
<connect gate="G$1" pin="P0.7_AD7" pad="30"/>
<connect gate="G$1" pin="P1.0" pad="40"/>
<connect gate="G$1" pin="P1.1" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5" pad="1"/>
<connect gate="G$1" pin="P1.6" pad="2"/>
<connect gate="G$1" pin="P1.7" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0/RXD" pad="5"/>
<connect gate="G$1" pin="P3.1/TXD" pad="7"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="8"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/!WR" pad="12"/>
<connect gate="G$1" pin="P3.7/!RD" pad="13"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="17"/>
</connects>
<technologies>
<technology name="-12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-16">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89S51-*" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 4K BytesIn-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2487.pdf</description>
<gates>
<gate name="P" symbol="AT89S51"/>
</gates>
<devices>
<device name="P" package="DIL40">
<connects>
<connect gate="P" pin="!EA!/VPP" pad="31"/>
<connect gate="P" pin="!PSEN" pad="29"/>
<connect gate="P" pin="ALE/!PROG" pad="30"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="P0.0_AD0" pad="39"/>
<connect gate="P" pin="P0.1_AD1" pad="38"/>
<connect gate="P" pin="P0.2_AD2" pad="37"/>
<connect gate="P" pin="P0.3_AD3" pad="36"/>
<connect gate="P" pin="P0.4_AD4" pad="35"/>
<connect gate="P" pin="P0.5_AD5" pad="34"/>
<connect gate="P" pin="P0.6_AD6" pad="33"/>
<connect gate="P" pin="P0.7_AD7" pad="32"/>
<connect gate="P" pin="P1.0" pad="1"/>
<connect gate="P" pin="P1.1" pad="2"/>
<connect gate="P" pin="P1.2" pad="3"/>
<connect gate="P" pin="P1.3" pad="4"/>
<connect gate="P" pin="P1.4" pad="5"/>
<connect gate="P" pin="P1.5_MOSI" pad="6"/>
<connect gate="P" pin="P1.6_MISO" pad="7"/>
<connect gate="P" pin="P1.7_SCK" pad="8"/>
<connect gate="P" pin="P2.0_A8" pad="21"/>
<connect gate="P" pin="P2.1_A9" pad="22"/>
<connect gate="P" pin="P2.2_A10" pad="23"/>
<connect gate="P" pin="P2.3_A11" pad="24"/>
<connect gate="P" pin="P2.4_A12" pad="25"/>
<connect gate="P" pin="P2.5_A13" pad="26"/>
<connect gate="P" pin="P2.6_A14" pad="27"/>
<connect gate="P" pin="P2.7_A15" pad="28"/>
<connect gate="P" pin="P3.0/RXD" pad="10"/>
<connect gate="P" pin="P3.1/TXD" pad="11"/>
<connect gate="P" pin="P3.2/!INT0" pad="12"/>
<connect gate="P" pin="P3.3/!INT1" pad="13"/>
<connect gate="P" pin="P3.4/T0" pad="14"/>
<connect gate="P" pin="P3.5/T1" pad="15"/>
<connect gate="P" pin="P3.6/!WR" pad="16"/>
<connect gate="P" pin="P3.7/!RD" pad="17"/>
<connect gate="P" pin="RST" pad="9"/>
<connect gate="P" pin="VCC" pad="40"/>
<connect gate="P" pin="XTAL1" pad="19"/>
<connect gate="P" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89S51-24PU"/>
<attribute name="OC_FARNELL" value="1095739"/>
<attribute name="OC_NEWARK" value="96K6578"/>
</technology>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89S51-24PU"/>
<attribute name="OC_FARNELL" value="1095739"/>
<attribute name="OC_NEWARK" value="96K6578"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC44">
<connects>
<connect gate="P" pin="!EA!/VPP" pad="35"/>
<connect gate="P" pin="!PSEN" pad="32"/>
<connect gate="P" pin="ALE/!PROG" pad="33"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="P0.0_AD0" pad="43"/>
<connect gate="P" pin="P0.1_AD1" pad="42"/>
<connect gate="P" pin="P0.2_AD2" pad="41"/>
<connect gate="P" pin="P0.3_AD3" pad="40"/>
<connect gate="P" pin="P0.4_AD4" pad="39"/>
<connect gate="P" pin="P0.5_AD5" pad="38"/>
<connect gate="P" pin="P0.6_AD6" pad="37"/>
<connect gate="P" pin="P0.7_AD7" pad="36"/>
<connect gate="P" pin="P1.0" pad="2"/>
<connect gate="P" pin="P1.1" pad="3"/>
<connect gate="P" pin="P1.2" pad="4"/>
<connect gate="P" pin="P1.3" pad="5"/>
<connect gate="P" pin="P1.4" pad="6"/>
<connect gate="P" pin="P1.5_MOSI" pad="7"/>
<connect gate="P" pin="P1.6_MISO" pad="8"/>
<connect gate="P" pin="P1.7_SCK" pad="9"/>
<connect gate="P" pin="P2.0_A8" pad="24"/>
<connect gate="P" pin="P2.1_A9" pad="25"/>
<connect gate="P" pin="P2.2_A10" pad="26"/>
<connect gate="P" pin="P2.3_A11" pad="27"/>
<connect gate="P" pin="P2.4_A12" pad="28"/>
<connect gate="P" pin="P2.5_A13" pad="29"/>
<connect gate="P" pin="P2.6_A14" pad="30"/>
<connect gate="P" pin="P2.7_A15" pad="31"/>
<connect gate="P" pin="P3.0/RXD" pad="11"/>
<connect gate="P" pin="P3.1/TXD" pad="13"/>
<connect gate="P" pin="P3.2/!INT0" pad="14"/>
<connect gate="P" pin="P3.3/!INT1" pad="15"/>
<connect gate="P" pin="P3.4/T0" pad="16"/>
<connect gate="P" pin="P3.5/T1" pad="17"/>
<connect gate="P" pin="P3.6/!WR" pad="18"/>
<connect gate="P" pin="P3.7/!RD" pad="19"/>
<connect gate="P" pin="RST" pad="10"/>
<connect gate="P" pin="VCC" pad="44"/>
<connect gate="P" pin="XTAL1" pad="21"/>
<connect gate="P" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89S51-24JU"/>
<attribute name="OC_FARNELL" value="1095738"/>
<attribute name="OC_NEWARK" value="96K6577"/>
</technology>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1095738"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="S44">
<connects>
<connect gate="P" pin="!EA!/VPP" pad="35"/>
<connect gate="P" pin="!PSEN" pad="32"/>
<connect gate="P" pin="ALE/!PROG" pad="33"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="P0.0_AD0" pad="43"/>
<connect gate="P" pin="P0.1_AD1" pad="42"/>
<connect gate="P" pin="P0.2_AD2" pad="41"/>
<connect gate="P" pin="P0.3_AD3" pad="40"/>
<connect gate="P" pin="P0.4_AD4" pad="39"/>
<connect gate="P" pin="P0.5_AD5" pad="38"/>
<connect gate="P" pin="P0.6_AD6" pad="37"/>
<connect gate="P" pin="P0.7_AD7" pad="36"/>
<connect gate="P" pin="P1.0" pad="2"/>
<connect gate="P" pin="P1.1" pad="3"/>
<connect gate="P" pin="P1.2" pad="4"/>
<connect gate="P" pin="P1.3" pad="5"/>
<connect gate="P" pin="P1.4" pad="6"/>
<connect gate="P" pin="P1.5_MOSI" pad="7"/>
<connect gate="P" pin="P1.6_MISO" pad="8"/>
<connect gate="P" pin="P1.7_SCK" pad="9"/>
<connect gate="P" pin="P2.0_A8" pad="24"/>
<connect gate="P" pin="P2.1_A9" pad="25"/>
<connect gate="P" pin="P2.2_A10" pad="26"/>
<connect gate="P" pin="P2.3_A11" pad="27"/>
<connect gate="P" pin="P2.4_A12" pad="28"/>
<connect gate="P" pin="P2.5_A13" pad="29"/>
<connect gate="P" pin="P2.6_A14" pad="30"/>
<connect gate="P" pin="P2.7_A15" pad="31"/>
<connect gate="P" pin="P3.0/RXD" pad="11"/>
<connect gate="P" pin="P3.1/TXD" pad="13"/>
<connect gate="P" pin="P3.2/!INT0" pad="14"/>
<connect gate="P" pin="P3.3/!INT1" pad="15"/>
<connect gate="P" pin="P3.4/T0" pad="16"/>
<connect gate="P" pin="P3.5/T1" pad="17"/>
<connect gate="P" pin="P3.6/!WR" pad="18"/>
<connect gate="P" pin="P3.7/!RD" pad="19"/>
<connect gate="P" pin="RST" pad="10"/>
<connect gate="P" pin="VCC" pad="44"/>
<connect gate="P" pin="XTAL1" pad="21"/>
<connect gate="P" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89S51*P" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 4K BytesIn-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2487.pdf</description>
<gates>
<gate name="G$1" symbol="AT89S51"/>
<gate name="P" symbol="GND"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE/!PROG" pad="27"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="P0.0_AD0" pad="37"/>
<connect gate="G$1" pin="P0.1_AD1" pad="36"/>
<connect gate="G$1" pin="P0.2_AD2" pad="35"/>
<connect gate="G$1" pin="P0.3_AD3" pad="34"/>
<connect gate="G$1" pin="P0.4_AD4" pad="33"/>
<connect gate="G$1" pin="P0.5_AD5" pad="32"/>
<connect gate="G$1" pin="P0.6_AD6" pad="31"/>
<connect gate="G$1" pin="P0.7_AD7" pad="30"/>
<connect gate="G$1" pin="P1.0" pad="40"/>
<connect gate="G$1" pin="P1.1" pad="41"/>
<connect gate="G$1" pin="P1.2" pad="42"/>
<connect gate="G$1" pin="P1.3" pad="43"/>
<connect gate="G$1" pin="P1.4" pad="44"/>
<connect gate="G$1" pin="P1.5_MOSI" pad="1"/>
<connect gate="G$1" pin="P1.6_MISO" pad="2"/>
<connect gate="G$1" pin="P1.7_SCK" pad="3"/>
<connect gate="G$1" pin="P2.0_A8" pad="18"/>
<connect gate="G$1" pin="P2.1_A9" pad="19"/>
<connect gate="G$1" pin="P2.2_A10" pad="20"/>
<connect gate="G$1" pin="P2.3_A11" pad="21"/>
<connect gate="G$1" pin="P2.4_A12" pad="22"/>
<connect gate="G$1" pin="P2.5_A13" pad="23"/>
<connect gate="G$1" pin="P2.6_A14" pad="24"/>
<connect gate="G$1" pin="P2.7_A15" pad="25"/>
<connect gate="G$1" pin="P3.0/RXD" pad="5"/>
<connect gate="G$1" pin="P3.1/TXD" pad="7"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="8"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="9"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="11"/>
<connect gate="G$1" pin="P3.6/!WR" pad="12"/>
<connect gate="G$1" pin="P3.7/!RD" pad="13"/>
<connect gate="G$1" pin="RST" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
<connect gate="P" pin="GND" pad="17"/>
</connects>
<technologies>
<technology name="-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-33">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T89C51CC02*-?IM" prefix="IC">
<description>&lt;b&gt;Enhanced 8-bit Microcontroller with CAN Controller and Flash&lt;/b&gt; 80C51 Core Architecture&lt;p&gt; 
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.</description>
<gates>
<gate name="G$1" symbol="T89C51CC02"/>
</gates>
<devices>
<device name="TIS" package="SO28W">
<connects>
<connect gate="G$1" pin="P1.0/AN0/T2" pad="28"/>
<connect gate="G$1" pin="P1.1/AN1/T2EX" pad="27"/>
<connect gate="G$1" pin="P1.2/AN2/ECI" pad="26"/>
<connect gate="G$1" pin="P1.3/AN3/CEX0" pad="25"/>
<connect gate="G$1" pin="P1.4/AN4/CEX1" pad="24"/>
<connect gate="G$1" pin="P1.5/AN5" pad="23"/>
<connect gate="G$1" pin="P1.6/AN6" pad="22"/>
<connect gate="G$1" pin="P1.7/AN7" pad="21"/>
<connect gate="G$1" pin="P2.0" pad="20"/>
<connect gate="G$1" pin="P2.1" pad="6"/>
<connect gate="G$1" pin="P3.0/RXD" pad="14"/>
<connect gate="G$1" pin="P3.1/TXD" pad="13"/>
<connect gate="G$1" pin="P3.2/!INT" pad="12"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="11"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="9"/>
<connect gate="G$1" pin="P3.6" pad="8"/>
<connect gate="G$1" pin="P3.7" pad="7"/>
<connect gate="G$1" pin="P4.0/RXDC" pad="5"/>
<connect gate="G$1" pin="P4.1/TXDC" pad="4"/>
<connect gate="G$1" pin="RST" pad="19"/>
<connect gate="G$1" pin="VAGND" pad="2"/>
<connect gate="G$1" pin="VAREF" pad="1"/>
<connect gate="G$1" pin="VAVCC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="17"/>
<connect gate="G$1" pin="VSS" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="16"/>
<connect gate="G$1" pin="XTAL2" pad="15"/>
</connects>
<technologies>
<technology name="CA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIL40/SOIC28ZIFAWM-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M9134"/>
</technology>
<technology name="UA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIL40/SOIC28ZIFAWM-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M9134"/>
</technology>
</technologies>
</device>
<device name="SIS" package="PLCC28">
<connects>
<connect gate="G$1" pin="P1.0/AN0/T2" pad="28"/>
<connect gate="G$1" pin="P1.1/AN1/T2EX" pad="27"/>
<connect gate="G$1" pin="P1.2/AN2/ECI" pad="26"/>
<connect gate="G$1" pin="P1.3/AN3/CEX0" pad="25"/>
<connect gate="G$1" pin="P1.4/AN4/CEX1" pad="24"/>
<connect gate="G$1" pin="P1.5/AN5" pad="23"/>
<connect gate="G$1" pin="P1.6/AN6" pad="22"/>
<connect gate="G$1" pin="P1.7/AN7" pad="21"/>
<connect gate="G$1" pin="P2.0" pad="20"/>
<connect gate="G$1" pin="P2.1" pad="6"/>
<connect gate="G$1" pin="P3.0/RXD" pad="14"/>
<connect gate="G$1" pin="P3.1/TXD" pad="13"/>
<connect gate="G$1" pin="P3.2/!INT" pad="12"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="11"/>
<connect gate="G$1" pin="P3.4/T0" pad="10"/>
<connect gate="G$1" pin="P3.5/T1" pad="9"/>
<connect gate="G$1" pin="P3.6" pad="8"/>
<connect gate="G$1" pin="P3.7" pad="7"/>
<connect gate="G$1" pin="P4.0/RXDC" pad="5"/>
<connect gate="G$1" pin="P4.1/TXDC" pad="4"/>
<connect gate="G$1" pin="RST" pad="19"/>
<connect gate="G$1" pin="VAGND" pad="2"/>
<connect gate="G$1" pin="VAREF" pad="1"/>
<connect gate="G$1" pin="VAVCC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="17"/>
<connect gate="G$1" pin="VSS" pad="18"/>
<connect gate="G$1" pin="XTAL1" pad="16"/>
<connect gate="G$1" pin="XTAL2" pad="15"/>
</connects>
<technologies>
<technology name="CA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIL40/PLCC28ZIFAWM-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M9105"/>
</technology>
<technology name="UA">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIL40/PLCC28ZIFAWM-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M9105"/>
</technology>
</technologies>
</device>
<device name="RAT" package="VQFP32">
<connects>
<connect gate="G$1" pin="P1.0/AN0/T2" pad="27"/>
<connect gate="G$1" pin="P1.1/AN1/T2EX" pad="26"/>
<connect gate="G$1" pin="P1.2/AN2/ECI" pad="25"/>
<connect gate="G$1" pin="P1.3/AN3/CEX0" pad="24"/>
<connect gate="G$1" pin="P1.4/AN4/CEX1" pad="23"/>
<connect gate="G$1" pin="P1.5/AN5" pad="22"/>
<connect gate="G$1" pin="P1.6/AN6" pad="21"/>
<connect gate="G$1" pin="P1.7/AN7" pad="20"/>
<connect gate="G$1" pin="P2.0" pad="19"/>
<connect gate="G$1" pin="P2.1" pad="2"/>
<connect gate="G$1" pin="P3.0/RXD" pad="11"/>
<connect gate="G$1" pin="P3.1/TXD" pad="10"/>
<connect gate="G$1" pin="P3.2/!INT" pad="9"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="8"/>
<connect gate="G$1" pin="P3.4/T0" pad="6"/>
<connect gate="G$1" pin="P3.5/T1" pad="5"/>
<connect gate="G$1" pin="P3.6" pad="4"/>
<connect gate="G$1" pin="P3.7" pad="3"/>
<connect gate="G$1" pin="P4.0/RXDC" pad="1"/>
<connect gate="G$1" pin="P4.1/TXDC" pad="32"/>
<connect gate="G$1" pin="RST" pad="17"/>
<connect gate="G$1" pin="VAGND" pad="29"/>
<connect gate="G$1" pin="VAREF" pad="28"/>
<connect gate="G$1" pin="VAVCC" pad="31"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="CA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="UA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T89C51CC02*-TDSIM" prefix="IC">
<description>&lt;b&gt;Enhanced 8-bit Microcontroller with CAN Controller and Flash&lt;/b&gt; 80C51 Core Architecture&lt;p&gt; 
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4126.</description>
<gates>
<gate name="G$1" symbol="T89C51CC02-SO24"/>
</gates>
<devices>
<device name="" package="SO24W">
<connects>
<connect gate="G$1" pin="P1.0/AN0/T2" pad="24"/>
<connect gate="G$1" pin="P1.1/AN1/T2EX" pad="23"/>
<connect gate="G$1" pin="P1.2/AN2/ECI" pad="22"/>
<connect gate="G$1" pin="P1.3/AN3/CEX0" pad="21"/>
<connect gate="G$1" pin="P1.4/AN4/CEX1" pad="20"/>
<connect gate="G$1" pin="P1.5/AN5" pad="19"/>
<connect gate="G$1" pin="P1.6/AN6" pad="18"/>
<connect gate="G$1" pin="P1.7/AN7" pad="17"/>
<connect gate="G$1" pin="P3.0/RXD" pad="11"/>
<connect gate="G$1" pin="P3.1/TXD" pad="10"/>
<connect gate="G$1" pin="P3.2/!INT" pad="9"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="8"/>
<connect gate="G$1" pin="P3.4/T0" pad="7"/>
<connect gate="G$1" pin="P3.5/T1" pad="6"/>
<connect gate="G$1" pin="P4.0/RXDC" pad="5"/>
<connect gate="G$1" pin="P4.1/TXDC" pad="4"/>
<connect gate="G$1" pin="RST" pad="16"/>
<connect gate="G$1" pin="VAGND" pad="2"/>
<connect gate="G$1" pin="VAREF" pad="1"/>
<connect gate="G$1" pin="VAVCC" pad="3"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VSS" pad="15"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="CA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="UA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91RM9200" prefix="IC">
<description>Auto generated by &lt;b&gt;make-symbol-device-package(bsdl).ulp&lt;/b&gt;&lt;p&gt;
Source: at91rm9200_bga.bsd</description>
<gates>
<gate name="G$1" symbol="AT91RM9200_BGA"/>
</gates>
<devices>
<device name="" package="LFBGA256_A_291X326">
<connects>
<connect gate="G$1" pin="A10_SDRAM" pad="N6"/>
<connect gate="G$1" pin="A16_BA0" pad="U3"/>
<connect gate="G$1" pin="A17_BA1" pad="T3"/>
<connect gate="G$1" pin="A1_DQM2" pad="M4"/>
<connect gate="G$1" pin="A_10" pad="M5"/>
<connect gate="G$1" pin="A_11" pad="P5"/>
<connect gate="G$1" pin="A_12" pad="P3"/>
<connect gate="G$1" pin="A_13" pad="P2"/>
<connect gate="G$1" pin="A_14" pad="N5"/>
<connect gate="G$1" pin="A_15" pad="T1"/>
<connect gate="G$1" pin="A_18" pad="R3"/>
<connect gate="G$1" pin="A_19" pad="U4"/>
<connect gate="G$1" pin="A_2" pad="M6"/>
<connect gate="G$1" pin="A_20" pad="R4"/>
<connect gate="G$1" pin="A_21" pad="N8"/>
<connect gate="G$1" pin="A_22" pad="P6"/>
<connect gate="G$1" pin="A_3" pad="M3"/>
<connect gate="G$1" pin="A_4" pad="N4"/>
<connect gate="G$1" pin="A_5" pad="N2"/>
<connect gate="G$1" pin="A_6" pad="L4"/>
<connect gate="G$1" pin="A_7" pad="P1"/>
<connect gate="G$1" pin="A_8" pad="N7"/>
<connect gate="G$1" pin="A_9" pad="N3"/>
<connect gate="G$1" pin="CAS" pad="U8"/>
<connect gate="G$1" pin="DM" pad="K2"/>
<connect gate="G$1" pin="DP" pad="K5"/>
<connect gate="G$1" pin="D_0" pad="R9"/>
<connect gate="G$1" pin="D_1" pad="P10"/>
<connect gate="G$1" pin="D_10" pad="P12"/>
<connect gate="G$1" pin="D_11" pad="U12"/>
<connect gate="G$1" pin="D_12" pad="T12"/>
<connect gate="G$1" pin="D_13" pad="R12"/>
<connect gate="G$1" pin="D_14" pad="U13"/>
<connect gate="G$1" pin="D_15" pad="P13"/>
<connect gate="G$1" pin="D_2" pad="N11"/>
<connect gate="G$1" pin="D_3" pad="U9"/>
<connect gate="G$1" pin="D_4" pad="M11"/>
<connect gate="G$1" pin="D_5" pad="P11"/>
<connect gate="G$1" pin="D_6" pad="U10"/>
<connect gate="G$1" pin="D_7" pad="U11"/>
<connect gate="G$1" pin="D_8" pad="R11"/>
<connect gate="G$1" pin="D_9" pad="T11"/>
<connect gate="G$1" pin="HDMA" pad="K3"/>
<connect gate="G$1" pin="HDMB" pad="L3"/>
<connect gate="G$1" pin="HDPA" pad="K1"/>
<connect gate="G$1" pin="HDPB" pad="L2"/>
<connect gate="G$1" pin="ICETCK" pad="E5"/>
<connect gate="G$1" pin="ICETDI" pad="A1"/>
<connect gate="G$1" pin="ICETDO" pad="B1"/>
<connect gate="G$1" pin="ICETMS" pad="C1"/>
<connect gate="G$1" pin="JTAGSEL" pad="A2"/>
<connect gate="G$1" pin="MIX33VDD@1" pad="P16"/>
<connect gate="G$1" pin="MIX33VDD@10" pad="D5"/>
<connect gate="G$1" pin="MIX33VDD@11" pad="D2"/>
<connect gate="G$1" pin="MIX33VDD@12" pad="D3"/>
<connect gate="G$1" pin="MIX33VDD@13" pad="H5"/>
<connect gate="G$1" pin="MIX33VDD@14" pad="K4"/>
<connect gate="G$1" pin="MIX33VDD@15" pad="L6"/>
<connect gate="G$1" pin="MIX33VDD@16" pad="M1"/>
<connect gate="G$1" pin="MIX33VDD@17" pad="P4"/>
<connect gate="G$1" pin="MIX33VDD@18" pad="R6"/>
<connect gate="G$1" pin="MIX33VDD@19" pad="T5"/>
<connect gate="G$1" pin="MIX33VDD@2" pad="R17"/>
<connect gate="G$1" pin="MIX33VDD@20" pad="R10"/>
<connect gate="G$1" pin="MIX33VDD@21" pad="R14"/>
<connect gate="G$1" pin="MIX33VDD@3" pad="K16"/>
<connect gate="G$1" pin="MIX33VDD@4" pad="H14"/>
<connect gate="G$1" pin="MIX33VDD@5" pad="A16"/>
<connect gate="G$1" pin="MIX33VDD@6" pad="A11"/>
<connect gate="G$1" pin="MIX33VDD@7" pad="B11"/>
<connect gate="G$1" pin="MIX33VDD@8" pad="D8"/>
<connect gate="G$1" pin="MIX33VDD@9" pad="A7"/>
<connect gate="G$1" pin="MIX33VSS@1" pad="M12"/>
<connect gate="G$1" pin="MIX33VSS@10" pad="E6"/>
<connect gate="G$1" pin="MIX33VSS@11" pad="D4"/>
<connect gate="G$1" pin="MIX33VSS@12" pad="E3"/>
<connect gate="G$1" pin="MIX33VSS@13" pad="G3"/>
<connect gate="G$1" pin="MIX33VSS@14" pad="L1"/>
<connect gate="G$1" pin="MIX33VSS@15" pad="L5"/>
<connect gate="G$1" pin="MIX33VSS@16" pad="M2"/>
<connect gate="G$1" pin="MIX33VSS@17" pad="R1"/>
<connect gate="G$1" pin="MIX33VSS@18" pad="M7"/>
<connect gate="G$1" pin="MIX33VSS@19" pad="U5"/>
<connect gate="G$1" pin="MIX33VSS@2" pad="P17"/>
<connect gate="G$1" pin="MIX33VSS@20" pad="T9"/>
<connect gate="G$1" pin="MIX33VSS@21" pad="T13"/>
<connect gate="G$1" pin="MIX33VSS@3" pad="J12"/>
<connect gate="G$1" pin="MIX33VSS@4" pad="H16"/>
<connect gate="G$1" pin="MIX33VSS@5" pad="C15"/>
<connect gate="G$1" pin="MIX33VSS@6" pad="C11"/>
<connect gate="G$1" pin="MIX33VSS@7" pad="D11"/>
<connect gate="G$1" pin="MIX33VSS@8" pad="B7"/>
<connect gate="G$1" pin="MIX33VSS@9" pad="E8"/>
<connect gate="G$1" pin="NBS3" pad="R8"/>
<connect gate="G$1" pin="NCS0_BFCS" pad="U6"/>
<connect gate="G$1" pin="NCS1_SDCS" pad="M9"/>
<connect gate="G$1" pin="NCS2" pad="T6"/>
<connect gate="G$1" pin="NCS3" pad="R7"/>
<connect gate="G$1" pin="NLBA0_DQM0" pad="N1"/>
<connect gate="G$1" pin="NRDNOE" pad="N9"/>
<connect gate="G$1" pin="NRST" pad="E1"/>
<connect gate="G$1" pin="NRW0NWE" pad="P8"/>
<connect gate="G$1" pin="NRW1_NUB_DQM1" pad="T7"/>
<connect gate="G$1" pin="NTRST" pad="E2"/>
<connect gate="G$1" pin="OSC32K_XIN" pad="G17"/>
<connect gate="G$1" pin="OSC32K_XOUT" pad="H17"/>
<connect gate="G$1" pin="OSC9M_XIN" pad="J17"/>
<connect gate="G$1" pin="OSC9M_XOUT" pad="K17"/>
<connect gate="G$1" pin="PA0" pad="G13"/>
<connect gate="G$1" pin="PA1" pad="G14"/>
<connect gate="G$1" pin="PA10" pad="D15"/>
<connect gate="G$1" pin="PA11" pad="B15"/>
<connect gate="G$1" pin="PA12" pad="B16"/>
<connect gate="G$1" pin="PA13" pad="A17"/>
<connect gate="G$1" pin="PA14" pad="A15"/>
<connect gate="G$1" pin="PA15" pad="B14"/>
<connect gate="G$1" pin="PA16" pad="D14"/>
<connect gate="G$1" pin="PA17" pad="B13"/>
<connect gate="G$1" pin="PA18" pad="C13"/>
<connect gate="G$1" pin="PA19" pad="A13"/>
<connect gate="G$1" pin="PA2" pad="G15"/>
<connect gate="G$1" pin="PA20" pad="C12"/>
<connect gate="G$1" pin="PA21" pad="D13"/>
<connect gate="G$1" pin="PA22" pad="D12"/>
<connect gate="G$1" pin="PA23" pad="A12"/>
<connect gate="G$1" pin="PA24" pad="B12"/>
<connect gate="G$1" pin="PA25" pad="E13"/>
<connect gate="G$1" pin="PA26" pad="E12"/>
<connect gate="G$1" pin="PA27" pad="G12"/>
<connect gate="G$1" pin="PA28" pad="F12"/>
<connect gate="G$1" pin="PA29" pad="E11"/>
<connect gate="G$1" pin="PA3" pad="G16"/>
<connect gate="G$1" pin="PA30" pad="F11"/>
<connect gate="G$1" pin="PA31" pad="A10"/>
<connect gate="G$1" pin="PA4" pad="F13"/>
<connect gate="G$1" pin="PA5" pad="F16"/>
<connect gate="G$1" pin="PA6" pad="E15"/>
<connect gate="G$1" pin="PA7" pad="B17"/>
<connect gate="G$1" pin="PA8" pad="C16"/>
<connect gate="G$1" pin="PA9" pad="E14"/>
<connect gate="G$1" pin="PB0" pad="B10"/>
<connect gate="G$1" pin="PB1" pad="C10"/>
<connect gate="G$1" pin="PB10" pad="B8"/>
<connect gate="G$1" pin="PB11" pad="F9"/>
<connect gate="G$1" pin="PB12" pad="C8"/>
<connect gate="G$1" pin="PB13" pad="C7"/>
<connect gate="G$1" pin="PB14" pad="D7"/>
<connect gate="G$1" pin="PB15" pad="E7"/>
<connect gate="G$1" pin="PB16" pad="F7"/>
<connect gate="G$1" pin="PB17" pad="A4"/>
<connect gate="G$1" pin="PB18" pad="B3"/>
<connect gate="G$1" pin="PB19" pad="C5"/>
<connect gate="G$1" pin="PB2" pad="D10"/>
<connect gate="G$1" pin="PB20" pad="A3"/>
<connect gate="G$1" pin="PB21" pad="B4"/>
<connect gate="G$1" pin="PB22" pad="C4"/>
<connect gate="G$1" pin="PB23" pad="F3"/>
<connect gate="G$1" pin="PB24" pad="F5"/>
<connect gate="G$1" pin="PB25" pad="F4"/>
<connect gate="G$1" pin="PB26" pad="G4"/>
<connect gate="G$1" pin="PB27" pad="G6"/>
<connect gate="G$1" pin="PB28" pad="J5"/>
<connect gate="G$1" pin="PB29" pad="J6"/>
<connect gate="G$1" pin="PB3" pad="E10"/>
<connect gate="G$1" pin="PB4" pad="A9"/>
<connect gate="G$1" pin="PB5" pad="B9"/>
<connect gate="G$1" pin="PB6" pad="C9"/>
<connect gate="G$1" pin="PB7" pad="E9"/>
<connect gate="G$1" pin="PB8" pad="D9"/>
<connect gate="G$1" pin="PB9" pad="A8"/>
<connect gate="G$1" pin="PC0" pad="M15"/>
<connect gate="G$1" pin="PC1" pad="M14"/>
<connect gate="G$1" pin="PC10" pad="L12"/>
<connect gate="G$1" pin="PC11" pad="N16"/>
<connect gate="G$1" pin="PC12" pad="N17"/>
<connect gate="G$1" pin="PC13" pad="M13"/>
<connect gate="G$1" pin="PC14" pad="M17"/>
<connect gate="G$1" pin="PC15" pad="L13"/>
<connect gate="G$1" pin="PC16" pad="U14"/>
<connect gate="G$1" pin="PC17" pad="R13"/>
<connect gate="G$1" pin="PC18" pad="U15"/>
<connect gate="G$1" pin="PC19" pad="T14"/>
<connect gate="G$1" pin="PC2" pad="L14"/>
<connect gate="G$1" pin="PC20" pad="U16"/>
<connect gate="G$1" pin="PC21" pad="T15"/>
<connect gate="G$1" pin="PC22" pad="U17"/>
<connect gate="G$1" pin="PC23" pad="T16"/>
<connect gate="G$1" pin="PC24" pad="R15"/>
<connect gate="G$1" pin="PC25" pad="T17"/>
<connect gate="G$1" pin="PC26" pad="P14"/>
<connect gate="G$1" pin="PC27" pad="P15"/>
<connect gate="G$1" pin="PC28" pad="N13"/>
<connect gate="G$1" pin="PC29" pad="R16"/>
<connect gate="G$1" pin="PC3" pad="L15"/>
<connect gate="G$1" pin="PC30" pad="N15"/>
<connect gate="G$1" pin="PC31" pad="N14"/>
<connect gate="G$1" pin="PC4" pad="K14"/>
<connect gate="G$1" pin="PC5" pad="K13"/>
<connect gate="G$1" pin="PC6" pad="K15"/>
<connect gate="G$1" pin="PC7" pad="T4"/>
<connect gate="G$1" pin="PC8" pad="R5"/>
<connect gate="G$1" pin="PC9" pad="P7"/>
<connect gate="G$1" pin="PD0" pad="E17"/>
<connect gate="G$1" pin="PD1" pad="F15"/>
<connect gate="G$1" pin="PD10" pad="C6"/>
<connect gate="G$1" pin="PD11" pad="A5"/>
<connect gate="G$1" pin="PD12" pad="B5"/>
<connect gate="G$1" pin="PD13" pad="B2"/>
<connect gate="G$1" pin="PD14" pad="C3"/>
<connect gate="G$1" pin="PD15" pad="C2"/>
<connect gate="G$1" pin="PD16" pad="F1"/>
<connect gate="G$1" pin="PD17" pad="G2"/>
<connect gate="G$1" pin="PD18" pad="G5"/>
<connect gate="G$1" pin="PD19" pad="G1"/>
<connect gate="G$1" pin="PD2" pad="F14"/>
<connect gate="G$1" pin="PD20" pad="H2"/>
<connect gate="G$1" pin="PD21" pad="H4"/>
<connect gate="G$1" pin="PD22" pad="H3"/>
<connect gate="G$1" pin="PD23" pad="H1"/>
<connect gate="G$1" pin="PD24" pad="J3"/>
<connect gate="G$1" pin="PD25" pad="J1"/>
<connect gate="G$1" pin="PD26" pad="J4"/>
<connect gate="G$1" pin="PD27" pad="J2"/>
<connect gate="G$1" pin="PD3" pad="E16"/>
<connect gate="G$1" pin="PD4" pad="D17"/>
<connect gate="G$1" pin="PD5" pad="C17"/>
<connect gate="G$1" pin="PD6" pad="D16"/>
<connect gate="G$1" pin="PD7" pad="D6"/>
<connect gate="G$1" pin="PD8" pad="A6"/>
<connect gate="G$1" pin="PD9" pad="B6"/>
<connect gate="G$1" pin="PLL_A_RC" pad="L17"/>
<connect gate="G$1" pin="PLL_B_RC" pad="F17"/>
<connect gate="G$1" pin="RAS" pad="N10"/>
<connect gate="G$1" pin="SDRAMCKE" pad="P9"/>
<connect gate="G$1" pin="SDRAMCLK" pad="U7"/>
<connect gate="G$1" pin="TST0" pad="E4"/>
<connect gate="G$1" pin="TST1" pad="D1"/>
<connect gate="G$1" pin="VDDI@1" pad="L16"/>
<connect gate="G$1" pin="VDDI@2" pad="C14"/>
<connect gate="G$1" pin="VDDI@3" pad="F6"/>
<connect gate="G$1" pin="VDDI@4" pad="U1"/>
<connect gate="G$1" pin="VDDI@5" pad="T2"/>
<connect gate="G$1" pin="VDDI@6" pad="T10"/>
<connect gate="G$1" pin="VDDI@7" pad="J15"/>
<connect gate="G$1" pin="VDDI@8" pad="J14"/>
<connect gate="G$1" pin="VDDI@9" pad="H13"/>
<connect gate="G$1" pin="VSSI@1" pad="M16"/>
<connect gate="G$1" pin="VSSI@2" pad="A14"/>
<connect gate="G$1" pin="VSSI@3" pad="F2"/>
<connect gate="G$1" pin="VSSI@4" pad="U2"/>
<connect gate="G$1" pin="VSSI@5" pad="R2"/>
<connect gate="G$1" pin="VSSI@6" pad="N12"/>
<connect gate="G$1" pin="VSSI@7" pad="J16"/>
<connect gate="G$1" pin="VSSI@8" pad="J13"/>
<connect gate="G$1" pin="VSSI@9" pad="H15"/>
<connect gate="G$1" pin="WE" pad="T8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT91RM9200-EK"/>
<attribute name="OC_FARNELL" value="1629536"/>
<attribute name="OC_NEWARK" value="02P6234"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATF16V8B" prefix="IC">
<description>&lt;b&gt;High perfomance CMOS (electrically erasable) programmable logic device (PLD)&lt;/b&gt;&lt;p&gt;
ABLE-Atmel-ABEL - P18V8R, P16V8C, P16V8AS, P17V8&lt;br&gt;
COPL Atmel-WinCUPL - G16V8MS, G16V8MA, G16V8AS, G16V8&lt;br&gt;
LOG/IC - GAL16V8_R, GAL16V8_G7, GAL16V8_C), GAL16V8&lt;br&gt;
Tango-PLD - G16V8R, G16V8C, G16V8AS, G16V8&lt;br&gt;


Source: http://www.atmel.com/dyn/resources/prod_documents/DOC0364.PDF</description>
<gates>
<gate name="G$1" symbol="ATF16V8B"/>
</gates>
<devices>
<device name="X" package="TSSOP20">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="O1" pad="19"/>
<connect gate="G$1" pin="O2" pad="18"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="15"/>
<connect gate="G$1" pin="O6" pad="14"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="J" package="PLCC20">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="O1" pad="19"/>
<connect gate="G$1" pin="O2" pad="18"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="15"/>
<connect gate="G$1" pin="O6" pad="14"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATF16V8CZ-15JU"/>
<attribute name="OC_FARNELL" value="1551767"/>
<attribute name="OC_NEWARK" value="94M6253"/>
</technology>
</technologies>
</device>
<device name="P3" package="DIL20">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="O1" pad="19"/>
<connect gate="G$1" pin="O2" pad="18"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="15"/>
<connect gate="G$1" pin="O6" pad="14"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATF16V8CZ-15PU"/>
<attribute name="OC_FARNELL" value="1551768"/>
<attribute name="OC_NEWARK" value="94M6254"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="I1" pad="2"/>
<connect gate="G$1" pin="I2" pad="3"/>
<connect gate="G$1" pin="I3" pad="4"/>
<connect gate="G$1" pin="I4" pad="5"/>
<connect gate="G$1" pin="I5" pad="6"/>
<connect gate="G$1" pin="I6" pad="7"/>
<connect gate="G$1" pin="I7" pad="8"/>
<connect gate="G$1" pin="I8" pad="9"/>
<connect gate="G$1" pin="O1" pad="19"/>
<connect gate="G$1" pin="O2" pad="18"/>
<connect gate="G$1" pin="O3" pad="17"/>
<connect gate="G$1" pin="O4" pad="16"/>
<connect gate="G$1" pin="O5" pad="15"/>
<connect gate="G$1" pin="O6" pad="14"/>
<connect gate="G$1" pin="O7" pad="13"/>
<connect gate="G$1" pin="O8" pad="12"/>
<connect gate="G$1" pin="OE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH, 1 kbytes SRAM, 512 bytes EEPROM, USART, 6-channel 10 bit ADC, 2-channel 8 bit ADC&lt;br&gt;
Pin compatible with Atmega48, ATMega88, ATMega168&lt;br&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="23-I/O"/>
</gates>
<devices>
<device name="-MI" package="MLF32">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA88PA-MU"/>
<attribute name="OC_FARNELL" value="1715491"/>
<attribute name="OC_NEWARK" value="15R0272"/>
</technology>
</technologies>
</device>
<device name="-AI" package="TQFP32-08">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="OC_NEWARK" value="73M8863"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH, 1 kbytes SRAM, 512 bytes EEPROM, USART, 4-channel 10 bit ADC, 2-channel 8 bit ADC&lt;br&gt;
Pin compatible with Atmega48, ATMega88, ATMega168&lt;br&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="23-I/O-2"/>
</gates>
<devices>
<device name="" package="DIL28-3">
<connects>
<connect gate="G$1" pin="AREF" pad="21"/>
<connect gate="G$1" pin="AVCC" pad="20"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PB0(ICP)" pad="14"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="15"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="16"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="17"/>
<connect gate="G$1" pin="PB4(MISO)" pad="18"/>
<connect gate="G$1" pin="PB5(SCK)" pad="19"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="9"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="10"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="1"/>
<connect gate="G$1" pin="PD0(RXD)" pad="2"/>
<connect gate="G$1" pin="PD1(TXD)" pad="3"/>
<connect gate="G$1" pin="PD2(INT0)" pad="4"/>
<connect gate="G$1" pin="PD3(INT1)" pad="5"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="6"/>
<connect gate="G$1" pin="PD5(T1)" pad="11"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="12"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA16" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M16-A"/>
</gates>
<devices>
<device name="-M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16MU"/>
<attribute name="OC_FARNELL" value="1455107"/>
<attribute name="OC_NEWARK" value="58M3723"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16AU"/>
<attribute name="OC_FARNELL" value="9171134"/>
<attribute name="OC_NEWARK" value="96K6515"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA16-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M16-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="31"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16PU"/>
<attribute name="OC_FARNELL" value="9171142"/>
<attribute name="OC_NEWARK" value="01M6885"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA32" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
Source: www.atmel.com .. doc2503.pdf</description>
<gates>
<gate name="G$1" symbol="32-I/O-M32-A"/>
</gates>
<devices>
<device name="-M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16MU"/>
<attribute name="OC_FARNELL" value="1455108"/>
<attribute name="OC_NEWARK" value="58M3733"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16AU"/>
<attribute name="OC_FARNELL" value="9171274"/>
<attribute name="OC_NEWARK" value="69K6677"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA32-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
Source: www.atmel.com .. doc2503.pdf</description>
<gates>
<gate name="G$1" symbol="32-I/O-M32-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="31"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16PU"/>
<attribute name="OC_FARNELL" value="1661729"/>
<attribute name="OC_NEWARK" value="51P1794"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA64" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
2 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA64"/>
</gates>
<devices>
<device name="-M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA64-16MU"/>
<attribute name="OC_FARNELL" value="1455120"/>
<attribute name="OC_NEWARK" value="58M3742"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA64-16AU"/>
<attribute name="OC_FARNELL" value="9171355"/>
<attribute name="OC_NEWARK" value="01M6899"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA128" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
128 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
4 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA128"/>
</gates>
<devices>
<device name="-M" package="MLF64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA128-16MU"/>
<attribute name="OC_FARNELL" value="1455093"/>
<attribute name="OC_NEWARK" value="58M3717"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA128-16AU"/>
<attribute name="OC_FARNELL" value="9171118"/>
<attribute name="OC_NEWARK" value="95K7364"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA169" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
4x25 Segment LCD Driver&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA169"/>
</gates>
<devices>
<device name="-M" package="MLF64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(MISO/PCINT11)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCINT10)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT12)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A/PCINT13)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCINT14)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCINT15)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCINT9)PB1" pad="11"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21/INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22/ICP)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(SS/PCINT8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(SEG14)" pad="33"/>
<connect gate="G$1" pin="PG1(SEG13)" pad="34"/>
<connect gate="G$1" pin="PG2(SEG4)" pad="43"/>
<connect gate="G$1" pin="PG3(T1/SEG24)" pad="18"/>
<connect gate="G$1" pin="PG4(T0/SEG23)" pad="19"/>
<connect gate="G$1" pin="PG5(RESET)" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-A" package="TQFP64">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(MISO/PCINT11)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCINT10)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT12)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A/PCINT13)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCINT14)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCINT15)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCINT9)PB1" pad="11"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21/INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22/ICP)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(SS/PCINT8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(SEG14)" pad="33"/>
<connect gate="G$1" pin="PG1(SEG13)" pad="34"/>
<connect gate="G$1" pin="PG2(SEG4)" pad="43"/>
<connect gate="G$1" pin="PG3(T1/SEG24)" pad="18"/>
<connect gate="G$1" pin="PG4(T0/SEG23)" pad="19"/>
<connect gate="G$1" pin="PG5(RESET)" pad="20"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA169PV-8AU"/>
<attribute name="OC_FARNELL" value="1617046"/>
<attribute name="OC_NEWARK" value="03P4011"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA323" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA323-A"/>
</gates>
<devices>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA323-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA323"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TCK)PC2" pad="24"/>
<connect gate="G$1" pin="(TDI)PC5" pad="27"/>
<connect gate="G$1" pin="(TDO)PC4" pad="26"/>
<connect gate="G$1" pin="(TMS)PC3" pad="25"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AGND" pad="31"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8515" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8515-A"/>
</gates>
<devices>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK)PD4" pad="10"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8515-16AU"/>
<attribute name="OC_FARNELL" value="9171410"/>
<attribute name="OC_NEWARK" value="01M6904"/>
</technology>
</technologies>
</device>
<device name="-M" package="MLF44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK)PD4" pad="10"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="26"/>
<connect gate="G$1" pin="(A11)PC3" pad="27"/>
<connect gate="G$1" pin="(A12)PC4" pad="28"/>
<connect gate="G$1" pin="(A13)PC5" pad="29"/>
<connect gate="G$1" pin="(A14)PC6" pad="30"/>
<connect gate="G$1" pin="(A15)PC7" pad="31"/>
<connect gate="G$1" pin="(A8)PC0" pad="24"/>
<connect gate="G$1" pin="(A9)PC1" pad="25"/>
<connect gate="G$1" pin="(AD0)PA0" pad="43"/>
<connect gate="G$1" pin="(AD1)PA1" pad="42"/>
<connect gate="G$1" pin="(AD2)PA2" pad="41"/>
<connect gate="G$1" pin="(AD3)PA3" pad="40"/>
<connect gate="G$1" pin="(AD4)PA4" pad="39"/>
<connect gate="G$1" pin="(AD5)PA5" pad="38"/>
<connect gate="G$1" pin="(AD6)PA6" pad="37"/>
<connect gate="G$1" pin="(AD7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="5"/>
<connect gate="G$1" pin="(INT0)PD2" pad="14"/>
<connect gate="G$1" pin="(INT1)PD3" pad="15"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="17"/>
<connect gate="G$1" pin="(RD)PD7" pad="19"/>
<connect gate="G$1" pin="(RXD)PD0" pad="11"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TXD)PD1" pad="13"/>
<connect gate="G$1" pin="(WR)PD6" pad="18"/>
<connect gate="G$1" pin="(XCK)PD4" pad="16"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="12"/>
<connect gate="G$1" pin="NC3" pad="23"/>
<connect gate="G$1" pin="NC4" pad="34"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="35"/>
<connect gate="G$1" pin="PE1(ALE)" pad="33"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="32"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8515-16JU"/>
<attribute name="OC_FARNELL" value="1562625"/>
<attribute name="OC_NEWARK" value="94M6261"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8515-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-7"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="23"/>
<connect gate="G$1" pin="(A11)PC3" pad="24"/>
<connect gate="G$1" pin="(A12)PC4" pad="25"/>
<connect gate="G$1" pin="(A13)PC5" pad="26"/>
<connect gate="G$1" pin="(A14)PC6" pad="27"/>
<connect gate="G$1" pin="(A15)PC7" pad="28"/>
<connect gate="G$1" pin="(A8)PC0" pad="21"/>
<connect gate="G$1" pin="(A9)PC1" pad="22"/>
<connect gate="G$1" pin="(AD0)PA0" pad="39"/>
<connect gate="G$1" pin="(AD1)PA1" pad="38"/>
<connect gate="G$1" pin="(AD2)PA2" pad="37"/>
<connect gate="G$1" pin="(AD3)PA3" pad="36"/>
<connect gate="G$1" pin="(AD4)PA4" pad="35"/>
<connect gate="G$1" pin="(AD5)PA5" pad="34"/>
<connect gate="G$1" pin="(AD6)PA6" pad="33"/>
<connect gate="G$1" pin="(AD7)PA7" pad="32"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="4"/>
<connect gate="G$1" pin="(INT0)PD2" pad="12"/>
<connect gate="G$1" pin="(INT1)PD3" pad="13"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="15"/>
<connect gate="G$1" pin="(RD)PD7" pad="17"/>
<connect gate="G$1" pin="(RXD)PD0" pad="10"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TXD)PD1" pad="11"/>
<connect gate="G$1" pin="(WR)PD6" pad="16"/>
<connect gate="G$1" pin="(XCK)PD4" pad="14"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="31"/>
<connect gate="G$1" pin="PE1(ALE)" pad="30"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="29"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8515-16PU"/>
<attribute name="OC_FARNELL" value="9171401"/>
<attribute name="OC_NEWARK" value="01M6905"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8535" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-A"/>
</gates>
<devices>
<device name="-A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8535-16AU"/>
<attribute name="OC_FARNELL" value="1528437"/>
<attribute name="OC_NEWARK" value="01M6908"/>
</technology>
</technologies>
</device>
<device name="-M" package="MLF44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-J" package="PLCC44">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="43"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="42"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="41"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="40"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="39"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="38"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="37"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="36"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="4"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="5"/>
<connect gate="G$1" pin="(ICP)PD6" pad="21"/>
<connect gate="G$1" pin="(INT0)PD2" pad="17"/>
<connect gate="G$1" pin="(INT1)PD3" pad="18"/>
<connect gate="G$1" pin="(MISO)PB6" pad="8"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="7"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="20"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="19"/>
<connect gate="G$1" pin="(OC2)PD7" pad="22"/>
<connect gate="G$1" pin="(RXD)PD0" pad="15"/>
<connect gate="G$1" pin="(SCK)PB7" pad="9"/>
<connect gate="G$1" pin="(SS)PB4" pad="6"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="2"/>
<connect gate="G$1" pin="(T1)PB1" pad="3"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="31"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="32"/>
<connect gate="G$1" pin="(TXD)PD1" pad="16"/>
<connect gate="G$1" pin="AREF" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="33"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="12"/>
<connect gate="G$1" pin="GND2" pad="24"/>
<connect gate="G$1" pin="GND@1" pad="34"/>
<connect gate="G$1" pin="PC0(SCL)" pad="25"/>
<connect gate="G$1" pin="PC1(SDA)" pad="26"/>
<connect gate="G$1" pin="PC2" pad="27"/>
<connect gate="G$1" pin="PC3" pad="28"/>
<connect gate="G$1" pin="PC4" pad="29"/>
<connect gate="G$1" pin="PC5" pad="30"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="XTAL1" pad="14"/>
<connect gate="G$1" pin="XTAL2" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8535-16JU"/>
<attribute name="OC_FARNELL" value="1562626"/>
<attribute name="OC_NEWARK" value="94M6263"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8535-P" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-P"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="40"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="39"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="38"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="37"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="36"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="35"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="34"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="33"/>
<connect gate="G$1" pin="(AIN0/OC0)PB2" pad="3"/>
<connect gate="G$1" pin="(AIN1/INT2)PB3" pad="4"/>
<connect gate="G$1" pin="(ICP)PD6" pad="20"/>
<connect gate="G$1" pin="(INT0)PD2" pad="16"/>
<connect gate="G$1" pin="(INT1)PD3" pad="17"/>
<connect gate="G$1" pin="(MISO)PB6" pad="7"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="6"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="19"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="18"/>
<connect gate="G$1" pin="(OC2)PD7" pad="21"/>
<connect gate="G$1" pin="(RXD)PD0" pad="14"/>
<connect gate="G$1" pin="(SCK)PB7" pad="8"/>
<connect gate="G$1" pin="(SCL)PC0" pad="22"/>
<connect gate="G$1" pin="(SDA)PC1" pad="23"/>
<connect gate="G$1" pin="(SS)PB4" pad="5"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="1"/>
<connect gate="G$1" pin="(T1)PB1" pad="2"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="28"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="29"/>
<connect gate="G$1" pin="(TXD)PD1" pad="15"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="31"/>
<connect gate="G$1" pin="PC2" pad="24"/>
<connect gate="G$1" pin="PC3" pad="25"/>
<connect gate="G$1" pin="PC4" pad="26"/>
<connect gate="G$1" pin="PC5" pad="27"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA8535-16PU"/>
<attribute name="OC_FARNELL" value="9171444"/>
<attribute name="OC_NEWARK" value="01M6909"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C513*-" prefix="IC">
<description>&lt;b&gt;8-bit Flash Microcontroller with Full Speed USB Device&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4136.pdf&lt;p&gt;
&lt;b&gt;&lt;i&gt;Data sheet mistake:&lt;/i&gt; &lt;/b&gt;define Packge type pin description for MLF48 but Order Number for QFN32 !?</description>
<gates>
<gate name="G$1" symbol="AT89C5131"/>
</gates>
<devices>
<device name="S" package="PLCC52">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="26"/>
<connect gate="G$1" pin="!PSEN" pad="28"/>
<connect gate="G$1" pin="!RST" pad="43"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="AVDD" pad="17"/>
<connect gate="G$1" pin="AVSS" pad="19"/>
<connect gate="G$1" pin="D+" pad="23"/>
<connect gate="G$1" pin="D-" pad="22"/>
<connect gate="G$1" pin="FREV" pad="24"/>
<connect gate="G$1" pin="P0.0_AD0" pad="52"/>
<connect gate="G$1" pin="P0.1_AD1" pad="45"/>
<connect gate="G$1" pin="P0.2_AD2" pad="44"/>
<connect gate="G$1" pin="P0.3_AD3" pad="42"/>
<connect gate="G$1" pin="P0.4_AD4" pad="40"/>
<connect gate="G$1" pin="P0.5_AD5" pad="38"/>
<connect gate="G$1" pin="P0.6_AD6" pad="37"/>
<connect gate="G$1" pin="P0.7_AD7" pad="36"/>
<connect gate="G$1" pin="P1.0/T2/KIN0" pad="47"/>
<connect gate="G$1" pin="P1.1/T2EX/KIN1/SS" pad="48"/>
<connect gate="G$1" pin="P1.2/ECI/KIN2" pad="49"/>
<connect gate="G$1" pin="P1.3/CEX0/KIN3" pad="50"/>
<connect gate="G$1" pin="P1.4/CEX1/KIN4" pad="51"/>
<connect gate="G$1" pin="P1.5/CEX2/KIN5/MISO" pad="4"/>
<connect gate="G$1" pin="P1.6/CEX3/KIN6/SCK" pad="5"/>
<connect gate="G$1" pin="P1.7/CEX4/KIN7/MOSI" pad="6"/>
<connect gate="G$1" pin="P2.0_A8" pad="1"/>
<connect gate="G$1" pin="P2.1_A9" pad="2"/>
<connect gate="G$1" pin="P2.2_A10" pad="3"/>
<connect gate="G$1" pin="P2.3_A11" pad="9"/>
<connect gate="G$1" pin="P2.4_A12" pad="10"/>
<connect gate="G$1" pin="P2.5_A13" pad="11"/>
<connect gate="G$1" pin="P2.6_A14" pad="14"/>
<connect gate="G$1" pin="P2.7_A15" pad="15"/>
<connect gate="G$1" pin="P3.0/RXD" pad="20"/>
<connect gate="G$1" pin="P3.1/TXD" pad="29"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="30"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="31"/>
<connect gate="G$1" pin="P3.4/T0" pad="32"/>
<connect gate="G$1" pin="P3.5/T1" pad="33"/>
<connect gate="G$1" pin="P3.6/!WR" pad="35"/>
<connect gate="G$1" pin="P3.7/!RD" pad="39"/>
<connect gate="G$1" pin="P4.0/SCL" pad="7"/>
<connect gate="G$1" pin="P4.1/SDA" pad="8"/>
<connect gate="G$1" pin="PLLF" pad="21"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="41"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT89C5131A-S3SUM"/>
<attribute name="OC_FARNELL" value="1095721"/>
<attribute name="OC_NEWARK" value="96K6570"/>
</technology>
</technologies>
</device>
<device name="R" package="VQFP64">
<connects>
<connect gate="G$1" pin="!EA!/VPP" pad="24"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="!RST" pad="44"/>
<connect gate="G$1" pin="ALE" pad="25"/>
<connect gate="G$1" pin="AVDD" pad="10"/>
<connect gate="G$1" pin="AVSS" pad="12"/>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="20"/>
<connect gate="G$1" pin="FREV" pad="22"/>
<connect gate="G$1" pin="P0.0_AD0" pad="55"/>
<connect gate="G$1" pin="P0.1_AD1" pad="46"/>
<connect gate="G$1" pin="P0.2_AD2" pad="45"/>
<connect gate="G$1" pin="P0.3_AD3" pad="43"/>
<connect gate="G$1" pin="P0.4_AD4" pad="40"/>
<connect gate="G$1" pin="P0.5_AD5" pad="38"/>
<connect gate="G$1" pin="P0.6_AD6" pad="37"/>
<connect gate="G$1" pin="P0.7_AD7" pad="36"/>
<connect gate="G$1" pin="P1.0/T2/KIN0" pad="50"/>
<connect gate="G$1" pin="P1.1/T2EX/KIN1/SS" pad="51"/>
<connect gate="G$1" pin="P1.2/ECI/KIN2" pad="52"/>
<connect gate="G$1" pin="P1.3/CEX0/KIN3" pad="53"/>
<connect gate="G$1" pin="P1.4/CEX1/KIN4" pad="54"/>
<connect gate="G$1" pin="P1.5/CEX2/KIN5/MISO" pad="59"/>
<connect gate="G$1" pin="P1.6/CEX3/KIN6/SCK" pad="60"/>
<connect gate="G$1" pin="P1.7/CEX4/KIN7/MOSI" pad="61"/>
<connect gate="G$1" pin="P2.0_A8" pad="56"/>
<connect gate="G$1" pin="P2.1_A9" pad="57"/>
<connect gate="G$1" pin="P2.2_A10" pad="58"/>
<connect gate="G$1" pin="P2.3_A11" pad="2"/>
<connect gate="G$1" pin="P2.4_A12" pad="3"/>
<connect gate="G$1" pin="P2.5_A13" pad="4"/>
<connect gate="G$1" pin="P2.6_A14" pad="7"/>
<connect gate="G$1" pin="P2.7_A15" pad="8"/>
<connect gate="G$1" pin="P3.0/RXD" pad="14"/>
<connect gate="G$1" pin="P3.1/TXD" pad="27"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="28"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="29"/>
<connect gate="G$1" pin="P3.4/T0" pad="30"/>
<connect gate="G$1" pin="P3.5/T1" pad="31"/>
<connect gate="G$1" pin="P3.6/!WR" pad="35"/>
<connect gate="G$1" pin="P3.7/!RD" pad="39"/>
<connect gate="G$1" pin="P4.0/SCL" pad="62"/>
<connect gate="G$1" pin="P4.1/SDA" pad="63"/>
<connect gate="G$1" pin="PLLF" pad="19"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VSS" pad="42"/>
<connect gate="G$1" pin="XTAL1" pad="6"/>
<connect gate="G$1" pin="XTAL2" pad="5"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT89C5132" prefix="IC">
<description>&lt;b&gt;USB Microcontroller with 64K Bytes Flash Memory&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4173.pdf</description>
<gates>
<gate name="G$1" symbol="AT89C5132"/>
</gates>
<devices>
<device name="" package="TQFP80">
<connects>
<connect gate="G$1" pin="!ISP" pad="2"/>
<connect gate="G$1" pin="!TST" pad="18"/>
<connect gate="G$1" pin="AIN0" pad="37"/>
<connect gate="G$1" pin="AIN1" pad="38"/>
<connect gate="G$1" pin="ALE" pad="1"/>
<connect gate="G$1" pin="AREFN" pad="36"/>
<connect gate="G$1" pin="AREFP" pad="35"/>
<connect gate="G$1" pin="AVDD" pad="33"/>
<connect gate="G$1" pin="AVSS" pad="34"/>
<connect gate="G$1" pin="D+" pad="21"/>
<connect gate="G$1" pin="D-" pad="22"/>
<connect gate="G$1" pin="DCLK" pad="44"/>
<connect gate="G$1" pin="DOUT" pad="43"/>
<connect gate="G$1" pin="DSEL" pad="45"/>
<connect gate="G$1" pin="FILT" pad="13"/>
<connect gate="G$1" pin="MCLK" pad="50"/>
<connect gate="G$1" pin="MCMD" pad="48"/>
<connect gate="G$1" pin="MDAT" pad="49"/>
<connect gate="G$1" pin="P0.0_AD0" pad="78"/>
<connect gate="G$1" pin="P0.1_AD1" pad="77"/>
<connect gate="G$1" pin="P0.2_AD2" pad="76"/>
<connect gate="G$1" pin="P0.3_AD3" pad="75"/>
<connect gate="G$1" pin="P0.4_AD4" pad="74"/>
<connect gate="G$1" pin="P0.5_AD5" pad="73"/>
<connect gate="G$1" pin="P0.6_AD6" pad="70"/>
<connect gate="G$1" pin="P0.7_AD7" pad="69"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="3"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="4"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="5"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="6"/>
<connect gate="G$1" pin="P1.4" pad="7"/>
<connect gate="G$1" pin="P1.5" pad="8"/>
<connect gate="G$1" pin="P1.6/SCL" pad="9"/>
<connect gate="G$1" pin="P1.7/SDA" pad="10"/>
<connect gate="G$1" pin="P2.0_A8" pad="64"/>
<connect gate="G$1" pin="P2.1_A9" pad="63"/>
<connect gate="G$1" pin="P2.2_A10" pad="58"/>
<connect gate="G$1" pin="P2.3_A11" pad="57"/>
<connect gate="G$1" pin="P2.4_A12" pad="56"/>
<connect gate="G$1" pin="P2.5_A13" pad="55"/>
<connect gate="G$1" pin="P2.6_A14" pad="54"/>
<connect gate="G$1" pin="P2.7_A15" pad="53"/>
<connect gate="G$1" pin="P3.0/RXD" pad="25"/>
<connect gate="G$1" pin="P3.1/TXD" pad="26"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="27"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="28"/>
<connect gate="G$1" pin="P3.4/T0" pad="29"/>
<connect gate="G$1" pin="P3.5/T1" pad="30"/>
<connect gate="G$1" pin="P3.6/!WR" pad="31"/>
<connect gate="G$1" pin="P3.7/!RD" pad="32"/>
<connect gate="G$1" pin="P4.0/MISO" pad="65"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="66"/>
<connect gate="G$1" pin="P4.2/SCK" pad="67"/>
<connect gate="G$1" pin="P4.3/!SS" pad="68"/>
<connect gate="G$1" pin="P4.4" pad="59"/>
<connect gate="G$1" pin="P4.5" pad="60"/>
<connect gate="G$1" pin="P4.6" pad="61"/>
<connect gate="G$1" pin="P4.7" pad="62"/>
<connect gate="G$1" pin="P5.0" pad="79"/>
<connect gate="G$1" pin="P5.1" pad="80"/>
<connect gate="G$1" pin="P5.2" pad="39"/>
<connect gate="G$1" pin="P5.3" pad="40"/>
<connect gate="G$1" pin="PVDD" pad="12"/>
<connect gate="G$1" pin="PVSS" pad="14"/>
<connect gate="G$1" pin="RST" pad="47"/>
<connect gate="G$1" pin="SCLK" pad="46"/>
<connect gate="G$1" pin="UVDD" pad="19"/>
<connect gate="G$1" pin="UVSS" pad="20"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="23"/>
<connect gate="G$1" pin="VDD@2" pad="41"/>
<connect gate="G$1" pin="VDD@3" pad="51"/>
<connect gate="G$1" pin="VDD@4" pad="71"/>
<connect gate="G$1" pin="VSS" pad="15"/>
<connect gate="G$1" pin="VSS@1" pad="24"/>
<connect gate="G$1" pin="VSS@2" pad="42"/>
<connect gate="G$1" pin="VSS@3" pad="52"/>
<connect gate="G$1" pin="VSS@4" pad="72"/>
<connect gate="G$1" pin="X1" pad="17"/>
<connect gate="G$1" pin="X2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="DEVELOP" package="PLCC84">
<connects>
<connect gate="G$1" pin="!ISP" pad="13"/>
<connect gate="G$1" pin="!TST" pad="30"/>
<connect gate="G$1" pin="AIN0" pad="49"/>
<connect gate="G$1" pin="AIN1" pad="50"/>
<connect gate="G$1" pin="ALE" pad="12"/>
<connect gate="G$1" pin="AREFN" pad="48"/>
<connect gate="G$1" pin="AREFP" pad="47"/>
<connect gate="G$1" pin="AVDD" pad="45"/>
<connect gate="G$1" pin="AVSS" pad="46"/>
<connect gate="G$1" pin="D+" pad="33"/>
<connect gate="G$1" pin="D-" pad="34"/>
<connect gate="G$1" pin="DCLK" pad="57"/>
<connect gate="G$1" pin="DOUT" pad="56"/>
<connect gate="G$1" pin="DSEL" pad="58"/>
<connect gate="G$1" pin="FILT" pad="24"/>
<connect gate="G$1" pin="MCLK" pad="63"/>
<connect gate="G$1" pin="MCMD" pad="61"/>
<connect gate="G$1" pin="MDAT" pad="62"/>
<connect gate="G$1" pin="P0.0_AD0" pad="8"/>
<connect gate="G$1" pin="P0.1_AD1" pad="7"/>
<connect gate="G$1" pin="P0.2_AD2" pad="6"/>
<connect gate="G$1" pin="P0.3_AD3" pad="5"/>
<connect gate="G$1" pin="P0.4_AD4" pad="4"/>
<connect gate="G$1" pin="P0.5_AD5" pad="3"/>
<connect gate="G$1" pin="P0.6_AD6" pad="84"/>
<connect gate="G$1" pin="P0.7_AD7" pad="83"/>
<connect gate="G$1" pin="P1.0/KIN0" pad="14"/>
<connect gate="G$1" pin="P1.1/KIN1" pad="15"/>
<connect gate="G$1" pin="P1.2/KIN2" pad="16"/>
<connect gate="G$1" pin="P1.3/KIN3" pad="17"/>
<connect gate="G$1" pin="P1.4" pad="18"/>
<connect gate="G$1" pin="P1.5" pad="19"/>
<connect gate="G$1" pin="P1.6/SCL" pad="20"/>
<connect gate="G$1" pin="P1.7/SDA" pad="21"/>
<connect gate="G$1" pin="P2.0_A8" pad="78"/>
<connect gate="G$1" pin="P2.1_A9" pad="77"/>
<connect gate="G$1" pin="P2.2_A10" pad="71"/>
<connect gate="G$1" pin="P2.3_A11" pad="70"/>
<connect gate="G$1" pin="P2.4_A12" pad="69"/>
<connect gate="G$1" pin="P2.5_A13" pad="68"/>
<connect gate="G$1" pin="P2.6_A14" pad="67"/>
<connect gate="G$1" pin="P2.7_A15" pad="66"/>
<connect gate="G$1" pin="P3.0/RXD" pad="37"/>
<connect gate="G$1" pin="P3.1/TXD" pad="38"/>
<connect gate="G$1" pin="P3.2/!INT0" pad="39"/>
<connect gate="G$1" pin="P3.3/!INT1" pad="40"/>
<connect gate="G$1" pin="P3.4/T0" pad="41"/>
<connect gate="G$1" pin="P3.5/T1" pad="42"/>
<connect gate="G$1" pin="P3.6/!WR" pad="43"/>
<connect gate="G$1" pin="P3.7/!RD" pad="44"/>
<connect gate="G$1" pin="P4.0/MISO" pad="79"/>
<connect gate="G$1" pin="P4.1/MOSI" pad="80"/>
<connect gate="G$1" pin="P4.2/SCK" pad="81"/>
<connect gate="G$1" pin="P4.3/!SS" pad="82"/>
<connect gate="G$1" pin="P4.4" pad="72"/>
<connect gate="G$1" pin="P4.5" pad="73"/>
<connect gate="G$1" pin="P4.6" pad="75"/>
<connect gate="G$1" pin="P4.7" pad="76"/>
<connect gate="G$1" pin="P5.0" pad="9"/>
<connect gate="G$1" pin="P5.1" pad="10"/>
<connect gate="G$1" pin="P5.2" pad="51"/>
<connect gate="G$1" pin="P5.3" pad="52"/>
<connect gate="G$1" pin="PVDD" pad="23"/>
<connect gate="G$1" pin="PVSS" pad="25"/>
<connect gate="G$1" pin="RST" pad="60"/>
<connect gate="G$1" pin="SCLK" pad="59"/>
<connect gate="G$1" pin="UVDD" pad="31"/>
<connect gate="G$1" pin="UVSS" pad="32"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="22"/>
<connect gate="G$1" pin="VDD@2" pad="35"/>
<connect gate="G$1" pin="VDD@3" pad="54"/>
<connect gate="G$1" pin="VDD@4" pad="64"/>
<connect gate="G$1" pin="VSS" pad="2"/>
<connect gate="G$1" pin="VSS@1" pad="26"/>
<connect gate="G$1" pin="VSS@2" pad="36"/>
<connect gate="G$1" pin="VSS@3" pad="55"/>
<connect gate="G$1" pin="VSS@4" pad="65"/>
<connect gate="G$1" pin="X1" pad="29"/>
<connect gate="G$1" pin="X2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8-MI" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH, 1 kbytes SRAM, 512 bytes EEPROM, USART, 6-channel 10 bit ADC, 2-channel 8 bit ADC&lt;br&gt;
Pin compatible with Atmega48, ATMega88, ATMega168&lt;br&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="23-I/O_MI"/>
</gates>
<devices>
<device name="" package="MLF32-TH">
<connects>
<connect gate="G$1" pin="ADC6" pad="19"/>
<connect gate="G$1" pin="ADC7" pad="22"/>
<connect gate="G$1" pin="AREF" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="GND@1" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="PB0(ICP)" pad="12"/>
<connect gate="G$1" pin="PB1(OC1A)" pad="13"/>
<connect gate="G$1" pin="PB2(SS/OC1B)" pad="14"/>
<connect gate="G$1" pin="PB3(MOSI/OC2)" pad="15"/>
<connect gate="G$1" pin="PB4(MISO)" pad="16"/>
<connect gate="G$1" pin="PB5(SCK)" pad="17"/>
<connect gate="G$1" pin="PB6(XTAL1/TOSC1)" pad="7"/>
<connect gate="G$1" pin="PB7(XTAL2/TOSC2)" pad="8"/>
<connect gate="G$1" pin="PC0(ADC0)" pad="23"/>
<connect gate="G$1" pin="PC1(ADC1)" pad="24"/>
<connect gate="G$1" pin="PC2(ADC2)" pad="25"/>
<connect gate="G$1" pin="PC3(ADC3)" pad="26"/>
<connect gate="G$1" pin="PC4(ADC4/SDA)" pad="27"/>
<connect gate="G$1" pin="PC5(ADC5/SCL)" pad="28"/>
<connect gate="G$1" pin="PC6(/RESET)" pad="29"/>
<connect gate="G$1" pin="PD0(RXD)" pad="30"/>
<connect gate="G$1" pin="PD1(TXD)" pad="31"/>
<connect gate="G$1" pin="PD2(INT0)" pad="32"/>
<connect gate="G$1" pin="PD3(INT1)" pad="1"/>
<connect gate="G$1" pin="PD4(XCK/T0)" pad="2"/>
<connect gate="G$1" pin="PD5(T1)" pad="9"/>
<connect gate="G$1" pin="PD6(AIN0)" pad="10"/>
<connect gate="G$1" pin="PD7(AIN1)" pad="11"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC@1" pad="4"/>
<connect gate="G$1" pin="VCC@2" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA88PA-MU"/>
<attribute name="OC_FARNELL" value="1715491"/>
<attribute name="OC_NEWARK" value="15R0272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA16-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M16-A_M"/>
</gates>
<devices>
<device name="" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16MU"/>
<attribute name="OC_FARNELL" value="1455097"/>
<attribute name="OC_NEWARK" value="58M3723"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA32-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
32 Kbytes FLASH&lt;br&gt;
2 Kbytes SRAM&lt;br&gt;
1 Kbytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
Source: www.atmel.com .. doc2503.pdf</description>
<gates>
<gate name="G$1" symbol="32-I/O-M32-A_M"/>
</gates>
<devices>
<device name="" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA32-16MU"/>
<attribute name="OC_FARNELL" value="1455108"/>
<attribute name="OC_NEWARK" value="58M3733"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA64-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
64 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
2 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA64-M"/>
</gates>
<devices>
<device name="" package="MLF64-TH">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA64-16MU"/>
<attribute name="OC_FARNELL" value="1455120"/>
<attribute name="OC_NEWARK" value="58M3742"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA128-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
128 Kbytes FLASH&lt;br&gt;
4 Kbytes SRAM&lt;br&gt;
4 Kbytes EEPROM&lt;br&gt;
DUAL USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA128-M"/>
</gates>
<devices>
<device name="" package="MLF64-TH">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="37"/>
<connect gate="G$1" pin="(A11)PC3" pad="38"/>
<connect gate="G$1" pin="(A12)PC4" pad="39"/>
<connect gate="G$1" pin="(A13)PC5" pad="40"/>
<connect gate="G$1" pin="(A14)PC6" pad="41"/>
<connect gate="G$1" pin="(A15)PC7" pad="42"/>
<connect gate="G$1" pin="(A8)PC0" pad="35"/>
<connect gate="G$1" pin="(A9)PC1" pad="36"/>
<connect gate="G$1" pin="(AD0)PA0" pad="51"/>
<connect gate="G$1" pin="(AD1)PA1" pad="50"/>
<connect gate="G$1" pin="(AD2)PA2" pad="49"/>
<connect gate="G$1" pin="(AD3)PA3" pad="48"/>
<connect gate="G$1" pin="(AD4)PA4" pad="47"/>
<connect gate="G$1" pin="(AD5)PA5" pad="46"/>
<connect gate="G$1" pin="(AD6)PA6" pad="45"/>
<connect gate="G$1" pin="(AD7)PA7" pad="44"/>
<connect gate="G$1" pin="(IC1)PD4" pad="29"/>
<connect gate="G$1" pin="(IC3/INT7)PE7" pad="9"/>
<connect gate="G$1" pin="(MISO)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2/OC1C)PB7" pad="17"/>
<connect gate="G$1" pin="(OC3A/AIN1)PE3" pad="5"/>
<connect gate="G$1" pin="(OC3B/INT4)PE4" pad="6"/>
<connect gate="G$1" pin="(OC3C/INT5)PE5" pad="7"/>
<connect gate="G$1" pin="(RXD/PDI)PE0" pad="2"/>
<connect gate="G$1" pin="(RXD1/INT2)PD2" pad="27"/>
<connect gate="G$1" pin="(SCK)PB1" pad="11"/>
<connect gate="G$1" pin="(SCL/INT0)PD0" pad="25"/>
<connect gate="G$1" pin="(SDA/INT1)PD1" pad="26"/>
<connect gate="G$1" pin="(SS)PB0" pad="10"/>
<connect gate="G$1" pin="(T1)PD6" pad="31"/>
<connect gate="G$1" pin="(T2)PD7" pad="32"/>
<connect gate="G$1" pin="(T3/INT6)PE6" pad="8"/>
<connect gate="G$1" pin="(TXD/PDO)PE1" pad="3"/>
<connect gate="G$1" pin="(TXD1/INT3)PD3" pad="28"/>
<connect gate="G$1" pin="(XCK0/AIN0)PE2" pad="4"/>
<connect gate="G$1" pin="(XCK1)PD5" pad="30"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="PEN" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(WR)" pad="33"/>
<connect gate="G$1" pin="PG1(RD)" pad="34"/>
<connect gate="G$1" pin="PG2(ALE)" pad="43"/>
<connect gate="G$1" pin="PG3(TOSC2)" pad="18"/>
<connect gate="G$1" pin="PG4(TOSC1)" pad="19"/>
<connect gate="G$1" pin="RESET" pad="20"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1" pad="24"/>
<connect gate="G$1" pin="XTAL2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA128-16MU"/>
<attribute name="OC_FARNELL" value="1455093"/>
<attribute name="OC_NEWARK" value="58M3717"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA169-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
16 Kbytes FLASH&lt;br&gt;
1 Kbytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;br&gt;
4x25 Segment LCD Driver&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="MEGA169-M"/>
</gates>
<devices>
<device name="" package="MLF64-TH">
<connects>
<connect gate="G$1" pin="(AIN1/PCINT3)PE3" pad="5"/>
<connect gate="G$1" pin="(CLKO/PCINT7)PE7" pad="9"/>
<connect gate="G$1" pin="(COM0)PA0" pad="51"/>
<connect gate="G$1" pin="(COM1)PA1" pad="50"/>
<connect gate="G$1" pin="(COM2)PA2" pad="49"/>
<connect gate="G$1" pin="(COM3)PA3" pad="48"/>
<connect gate="G$1" pin="(DI/SDA/PCINT5)PE5" pad="7"/>
<connect gate="G$1" pin="(DO/PCINT6)PE6" pad="8"/>
<connect gate="G$1" pin="(MISO/PCINT11)PB3" pad="13"/>
<connect gate="G$1" pin="(MOSI/PCINT10)PB2" pad="12"/>
<connect gate="G$1" pin="(OC0A/PCINT12)PB4" pad="14"/>
<connect gate="G$1" pin="(OC1A/PCINT13)PB5" pad="15"/>
<connect gate="G$1" pin="(OC1B/PCINT14)PB6" pad="16"/>
<connect gate="G$1" pin="(OC2A/PCINT15)PB7" pad="17"/>
<connect gate="G$1" pin="(RXD/PCINT0)PE0" pad="2"/>
<connect gate="G$1" pin="(SCK/PCINT9)PB1" pad="11"/>
<connect gate="G$1" pin="(SEG0)PA4" pad="47"/>
<connect gate="G$1" pin="(SEG1)PA5" pad="46"/>
<connect gate="G$1" pin="(SEG10)PC2" pad="37"/>
<connect gate="G$1" pin="(SEG11)PC1" pad="36"/>
<connect gate="G$1" pin="(SEG12)PC0" pad="35"/>
<connect gate="G$1" pin="(SEG15)PD7" pad="32"/>
<connect gate="G$1" pin="(SEG16)PD6" pad="31"/>
<connect gate="G$1" pin="(SEG17)PD5" pad="30"/>
<connect gate="G$1" pin="(SEG18)PD4" pad="29"/>
<connect gate="G$1" pin="(SEG19)PD3" pad="28"/>
<connect gate="G$1" pin="(SEG2)PA6" pad="45"/>
<connect gate="G$1" pin="(SEG20)PD2" pad="27"/>
<connect gate="G$1" pin="(SEG21/INT0)PD1" pad="26"/>
<connect gate="G$1" pin="(SEG22/ICP)PD0" pad="25"/>
<connect gate="G$1" pin="(SEG3)PA7" pad="44"/>
<connect gate="G$1" pin="(SEG5)PC7" pad="42"/>
<connect gate="G$1" pin="(SEG6)PC6" pad="41"/>
<connect gate="G$1" pin="(SEG7)PC5" pad="40"/>
<connect gate="G$1" pin="(SEG8)PC4" pad="39"/>
<connect gate="G$1" pin="(SEG9)PC3" pad="38"/>
<connect gate="G$1" pin="(SS/PCINT8)PB0" pad="10"/>
<connect gate="G$1" pin="(TXD/PCINT1)PE1" pad="3"/>
<connect gate="G$1" pin="(USCK/SCL/PCINT4)PE4" pad="6"/>
<connect gate="G$1" pin="(XCK0/AIN0/PCINT2)PE2" pad="4"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="63"/>
<connect gate="G$1" pin="GND@2" pad="53"/>
<connect gate="G$1" pin="LCDCAP" pad="1"/>
<connect gate="G$1" pin="PF0(ADC0)" pad="61"/>
<connect gate="G$1" pin="PF1(ADC1)" pad="60"/>
<connect gate="G$1" pin="PF2(ADC2)" pad="59"/>
<connect gate="G$1" pin="PF3(ADC3)" pad="58"/>
<connect gate="G$1" pin="PF4(ADC4/TCK)" pad="57"/>
<connect gate="G$1" pin="PF5(ADC5/TMS)" pad="56"/>
<connect gate="G$1" pin="PF6(ADC6/TDO)" pad="55"/>
<connect gate="G$1" pin="PF7(ADC7/TDI)" pad="54"/>
<connect gate="G$1" pin="PG0(SEG14)" pad="33"/>
<connect gate="G$1" pin="PG1(SEG13)" pad="34"/>
<connect gate="G$1" pin="PG2(SEG4)" pad="43"/>
<connect gate="G$1" pin="PG3(T1/SEG24)" pad="18"/>
<connect gate="G$1" pin="PG4(T0/SEG23)" pad="19"/>
<connect gate="G$1" pin="PG5(RESET)" pad="20"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XTAL1(TOSC1)" pad="24"/>
<connect gate="G$1" pin="XTAL2(TOSC2)" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8515-M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8515-A_M"/>
</gates>
<devices>
<device name="-M" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(A10)PC2" pad="20"/>
<connect gate="G$1" pin="(A11)PC3" pad="21"/>
<connect gate="G$1" pin="(A12)PC4" pad="22"/>
<connect gate="G$1" pin="(A13)PC5" pad="23"/>
<connect gate="G$1" pin="(A14)PC6" pad="24"/>
<connect gate="G$1" pin="(A15)PC7" pad="25"/>
<connect gate="G$1" pin="(A8)PC0" pad="18"/>
<connect gate="G$1" pin="(A9)PC1" pad="19"/>
<connect gate="G$1" pin="(AD0)PA0" pad="37"/>
<connect gate="G$1" pin="(AD1)PA1" pad="36"/>
<connect gate="G$1" pin="(AD2)PA2" pad="35"/>
<connect gate="G$1" pin="(AD3)PA3" pad="34"/>
<connect gate="G$1" pin="(AD4)PA4" pad="33"/>
<connect gate="G$1" pin="(AD5)PA5" pad="32"/>
<connect gate="G$1" pin="(AD6)PA6" pad="31"/>
<connect gate="G$1" pin="(AD7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(INT0)PD2" pad="8"/>
<connect gate="G$1" pin="(INT1)PD3" pad="9"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="11"/>
<connect gate="G$1" pin="(RD)PD7" pad="13"/>
<connect gate="G$1" pin="(RXD)PD0" pad="5"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/OC0)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TXD)PD1" pad="7"/>
<connect gate="G$1" pin="(WR)PD6" pad="12"/>
<connect gate="G$1" pin="(XCK)PD4" pad="10"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="17"/>
<connect gate="G$1" pin="NC3" pad="28"/>
<connect gate="G$1" pin="NC4" pad="39"/>
<connect gate="G$1" pin="PE0(ICP/INT2)" pad="29"/>
<connect gate="G$1" pin="PE1(ALE)" pad="27"/>
<connect gate="G$1" pin="PE2(OC1B)" pad="26"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEGA8535_M" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
8 Kbytes FLASH&lt;br&gt;
512 bytes SRAM&lt;br&gt;
512 bytes EEPROM&lt;br&gt;
USART&lt;br&gt;
8-channel 10 bit ADC&lt;p&gt;
Source: avr.lbr</description>
<gates>
<gate name="G$1" symbol="32-I/O-M8535-A_M"/>
</gates>
<devices>
<device name="-M" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(AIN0/INT2)PB2" pad="42"/>
<connect gate="G$1" pin="(AIN1/OC0)PB3" pad="43"/>
<connect gate="G$1" pin="(ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(OC2)PD7" pad="16"/>
<connect gate="G$1" pin="(RXD)PD0" pad="9"/>
<connect gate="G$1" pin="(SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(SS)PB4" pad="44"/>
<connect gate="G$1" pin="(T0/XCK)PB0" pad="40"/>
<connect gate="G$1" pin="(T1)PB1" pad="41"/>
<connect gate="G$1" pin="(TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(TXD)PD1" pad="10"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="39"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="PC0(SCL)" pad="19"/>
<connect gate="G$1" pin="PC1(SDA)" pad="20"/>
<connect gate="G$1" pin="PC2" pad="21"/>
<connect gate="G$1" pin="PC3" pad="22"/>
<connect gate="G$1" pin="PC4" pad="23"/>
<connect gate="G$1" pin="PC5" pad="24"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC1" pad="17"/>
<connect gate="G$1" pin="VCC2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY26*-M" prefix="IC">
<description>&lt;b&gt;8-bit AVR Microcontroller with 2K Bytes Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com .. doc1477.pdf</description>
<gates>
<gate name="G$1" symbol="TINY26_M"/>
</gates>
<devices>
<device name="" package="MLF32-TH">
<connects>
<connect gate="G$1" pin="(ADC0)PA0" pad="26"/>
<connect gate="G$1" pin="(ADC1)PA1" pad="25"/>
<connect gate="G$1" pin="(ADC10/!RESET!)PB7" pad="11"/>
<connect gate="G$1" pin="(ADC2)PA2" pad="23"/>
<connect gate="G$1" pin="(ADC3)PA4" pad="17"/>
<connect gate="G$1" pin="(ADC4)PA5" pad="15"/>
<connect gate="G$1" pin="(ADC5/AIN0)PA6" pad="14"/>
<connect gate="G$1" pin="(ADC6/AIN1)PA7" pad="13"/>
<connect gate="G$1" pin="(ADC7/XTAL1)PB4" pad="7"/>
<connect gate="G$1" pin="(ADC8/XTAL2)PB5" pad="8"/>
<connect gate="G$1" pin="(ADC9/INT0/T0)PB6" pad="10"/>
<connect gate="G$1" pin="(AREF)PA3" pad="22"/>
<connect gate="G$1" pin="(MISO/DO/OC1A)PB1" pad="31"/>
<connect gate="G$1" pin="(MOSI/DI/SDA/!OC1A!)PB0" pad="30"/>
<connect gate="G$1" pin="(OC1B)PB3" pad="2"/>
<connect gate="G$1" pin="(SCK/SCL/!OC1B!)PB2" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="18"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="21"/>
<connect gate="G$1" pin="THERMAL" pad="TH"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA644" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller&lt;/b&gt; with 64K Bytes In-System Programmable Flash&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2593.pdf</description>
<gates>
<gate name="G$1" symbol="ATMEGA644"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="(PCINT0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCINT1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCINT10/INT2/AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(PCINT11/OC0A/AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(PCINT12/OC0B/!SS!)PB4" pad="44"/>
<connect gate="G$1" pin="(PCINT13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCINT14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCINT15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCINT16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCINT17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCINT18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCINT19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCINT2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCINT20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCINT21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCINT22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCINT23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCINT24/RXD0)PD0" pad="9"/>
<connect gate="G$1" pin="(PCINT25/TXD0)PD1" pad="10"/>
<connect gate="G$1" pin="(PCINT26/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCINT27/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCINT28/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCINT29/OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCINT3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCINT30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCINT31/OC2A)PD7" pad="16"/>
<connect gate="G$1" pin="(PCINT4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCINT5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCINT6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCINT7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCINT8/XCK0/T0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCINT9/CLKO/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="17"/>
<connect gate="G$1" pin="VCC@2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644PV-10AU"/>
<attribute name="OC_FARNELL" value="1455123"/>
<attribute name="OC_NEWARK" value="58M3748"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA644*" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller&lt;/b&gt; with 64K Bytes In-System Programmable Flash&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2593.pdf</description>
<gates>
<gate name="G$1" symbol="ATMEGA644E"/>
</gates>
<devices>
<device name="M" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="(PCINT0/ADC0)PA0" pad="37"/>
<connect gate="G$1" pin="(PCINT1/ADC1)PA1" pad="36"/>
<connect gate="G$1" pin="(PCINT10/INT2/AIN0)PB2" pad="42"/>
<connect gate="G$1" pin="(PCINT11/OC0A/AIN1)PB3" pad="43"/>
<connect gate="G$1" pin="(PCINT12/OC0B/!SS!)PB4" pad="44"/>
<connect gate="G$1" pin="(PCINT13/MOSI)PB5" pad="1"/>
<connect gate="G$1" pin="(PCINT14/MISO)PB6" pad="2"/>
<connect gate="G$1" pin="(PCINT15/SCK)PB7" pad="3"/>
<connect gate="G$1" pin="(PCINT16/SCL)PC0" pad="19"/>
<connect gate="G$1" pin="(PCINT17/SDA)PC1" pad="20"/>
<connect gate="G$1" pin="(PCINT18/TCK)PC2" pad="21"/>
<connect gate="G$1" pin="(PCINT19/TMS)PC3" pad="22"/>
<connect gate="G$1" pin="(PCINT2/ADC2)PA2" pad="35"/>
<connect gate="G$1" pin="(PCINT20/TDO)PC4" pad="23"/>
<connect gate="G$1" pin="(PCINT21/TDI)PC5" pad="24"/>
<connect gate="G$1" pin="(PCINT22/TOSC1)PC6" pad="25"/>
<connect gate="G$1" pin="(PCINT23/TOSC2)PC7" pad="26"/>
<connect gate="G$1" pin="(PCINT24/RXD0)PD0" pad="9"/>
<connect gate="G$1" pin="(PCINT25/TXD0)PD1" pad="10"/>
<connect gate="G$1" pin="(PCINT26/INT0)PD2" pad="11"/>
<connect gate="G$1" pin="(PCINT27/INT1)PD3" pad="12"/>
<connect gate="G$1" pin="(PCINT28/OC1B)PD4" pad="13"/>
<connect gate="G$1" pin="(PCINT29/OC1A)PD5" pad="14"/>
<connect gate="G$1" pin="(PCINT3/ADC3)PA3" pad="34"/>
<connect gate="G$1" pin="(PCINT30/OC2B/ICP)PD6" pad="15"/>
<connect gate="G$1" pin="(PCINT31/OC2A)PD7" pad="16"/>
<connect gate="G$1" pin="(PCINT4/ADC4)PA4" pad="33"/>
<connect gate="G$1" pin="(PCINT5/ADC5)PA5" pad="32"/>
<connect gate="G$1" pin="(PCINT6/ADC6)PA6" pad="31"/>
<connect gate="G$1" pin="(PCINT7/ADC7)PA7" pad="30"/>
<connect gate="G$1" pin="(PCINT8/XCK0/T0)PB0" pad="40"/>
<connect gate="G$1" pin="(PCINT9/CLKO/T1)PB1" pad="41"/>
<connect gate="G$1" pin="AREF" pad="29"/>
<connect gate="G$1" pin="AVCC" pad="27"/>
<connect gate="G$1" pin="EXP" pad="TH"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="39"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VCC@1" pad="17"/>
<connect gate="G$1" pin="VCC@2" pad="38"/>
<connect gate="G$1" pin="XTAL1" pad="8"/>
<connect gate="G$1" pin="XTAL2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644P-20MU"/>
<attribute name="OC_FARNELL" value="1748528"/>
<attribute name="OC_NEWARK" value="26R5636"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91SAM7X*-AU" prefix="IC">
<description>&lt;b&gt;Highly integrated Flash microcontrollers based on the 32-bit ARM RISC processor&lt;/b&gt;&lt;p&gt;
512/256/128 Kbyte high-speed Flash and 128/64/32 Kbyte SRAM, a large set of peripherals, including an 802.3 Ethernet MAC and a CAN controller&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/6120s.pdf</description>
<gates>
<gate name="G$1" symbol="AT91SAM7X"/>
</gates>
<devices>
<device name="" package="LQFP100">
<connects>
<connect gate="G$1" pin="AD4" pad="3"/>
<connect gate="G$1" pin="AD5" pad="4"/>
<connect gate="G$1" pin="AD6" pad="5"/>
<connect gate="G$1" pin="AD7" pad="6"/>
<connect gate="G$1" pin="ADVREF" pad="1"/>
<connect gate="G$1" pin="DDM" pad="93"/>
<connect gate="G$1" pin="DDP" pad="94"/>
<connect gate="G$1" pin="ERASE" pad="92"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="16"/>
<connect gate="G$1" pin="GND@3" pad="32"/>
<connect gate="G$1" pin="GND@4" pad="52"/>
<connect gate="G$1" pin="GND@5" pad="68"/>
<connect gate="G$1" pin="GND@6" pad="83"/>
<connect gate="G$1" pin="GND@7" pad="96"/>
<connect gate="G$1" pin="JTAGSEL" pad="77"/>
<connect gate="G$1" pin="NRST" pad="57"/>
<connect gate="G$1" pin="PA0/PGMEN0" pad="81"/>
<connect gate="G$1" pin="PA1/PGMEN1" pad="82"/>
<connect gate="G$1" pin="PA10/PGMM2" pad="18"/>
<connect gate="G$1" pin="PA11/PGMM3" pad="19"/>
<connect gate="G$1" pin="PA12/PGMD0" pad="20"/>
<connect gate="G$1" pin="PA13/PGMD1" pad="21"/>
<connect gate="G$1" pin="PA14/PGMD2" pad="22"/>
<connect gate="G$1" pin="PA15/PGMD3" pad="23"/>
<connect gate="G$1" pin="PA16/PGMD4" pad="24"/>
<connect gate="G$1" pin="PA17/PGMD5" pad="25"/>
<connect gate="G$1" pin="PA18/PGMD6" pad="26"/>
<connect gate="G$1" pin="PA19/PGMD7" pad="46"/>
<connect gate="G$1" pin="PA2" pad="86"/>
<connect gate="G$1" pin="PA20/PGMD8" pad="47"/>
<connect gate="G$1" pin="PA21/PGMD9" pad="49"/>
<connect gate="G$1" pin="PA22/PGMD10" pad="50"/>
<connect gate="G$1" pin="PA23/PGMD11" pad="55"/>
<connect gate="G$1" pin="PA24/PGMD12" pad="56"/>
<connect gate="G$1" pin="PA25/PGMD13" pad="59"/>
<connect gate="G$1" pin="PA26/PGMD14" pad="60"/>
<connect gate="G$1" pin="PA27/PGMD15" pad="73"/>
<connect gate="G$1" pin="PA28" pad="74"/>
<connect gate="G$1" pin="PA29" pad="75"/>
<connect gate="G$1" pin="PA3" pad="85"/>
<connect gate="G$1" pin="PA30" pad="80"/>
<connect gate="G$1" pin="PA4/PGMNCMD" pad="88"/>
<connect gate="G$1" pin="PA5/PGMRDY" pad="89"/>
<connect gate="G$1" pin="PA6/PGMNOE" pad="90"/>
<connect gate="G$1" pin="PA7/PGMNVALID" pad="91"/>
<connect gate="G$1" pin="PA8/PGMM0" pad="13"/>
<connect gate="G$1" pin="PA9/PGMM1" pad="14"/>
<connect gate="G$1" pin="PB0" pad="40"/>
<connect gate="G$1" pin="PB1" pad="41"/>
<connect gate="G$1" pin="PB10" pad="44"/>
<connect gate="G$1" pin="PB11" pad="45"/>
<connect gate="G$1" pin="PB12" pad="39"/>
<connect gate="G$1" pin="PB13" pad="30"/>
<connect gate="G$1" pin="PB14" pad="29"/>
<connect gate="G$1" pin="PB15" pad="35"/>
<connect gate="G$1" pin="PB16" pad="53"/>
<connect gate="G$1" pin="PB17" pad="36"/>
<connect gate="G$1" pin="PB18" pad="63"/>
<connect gate="G$1" pin="PB19" pad="64"/>
<connect gate="G$1" pin="PB2" pad="42"/>
<connect gate="G$1" pin="PB20" pad="65"/>
<connect gate="G$1" pin="PB21" pad="66"/>
<connect gate="G$1" pin="PB22" pad="67"/>
<connect gate="G$1" pin="PB23" pad="69"/>
<connect gate="G$1" pin="PB24" pad="70"/>
<connect gate="G$1" pin="PB25" pad="71"/>
<connect gate="G$1" pin="PB26" pad="72"/>
<connect gate="G$1" pin="PB27/AD0" pad="9"/>
<connect gate="G$1" pin="PB28/AD1" pad="10"/>
<connect gate="G$1" pin="PB29/AD2" pad="11"/>
<connect gate="G$1" pin="PB3" pad="43"/>
<connect gate="G$1" pin="PB30/AD3" pad="12"/>
<connect gate="G$1" pin="PB4" pad="54"/>
<connect gate="G$1" pin="PB5" pad="34"/>
<connect gate="G$1" pin="PB6" pad="31"/>
<connect gate="G$1" pin="PB7" pad="38"/>
<connect gate="G$1" pin="PB8" pad="28"/>
<connect gate="G$1" pin="PB9" pad="27"/>
<connect gate="G$1" pin="PLLRC" pad="99"/>
<connect gate="G$1" pin="TCK" pad="79"/>
<connect gate="G$1" pin="TDI" pad="51"/>
<connect gate="G$1" pin="TDO" pad="76"/>
<connect gate="G$1" pin="TMS" pad="78"/>
<connect gate="G$1" pin="TST" pad="58"/>
<connect gate="G$1" pin="VDDCORE@1" pad="15"/>
<connect gate="G$1" pin="VDDCORE@2" pad="37"/>
<connect gate="G$1" pin="VDDCORE@3" pad="62"/>
<connect gate="G$1" pin="VDDCORE@4" pad="87"/>
<connect gate="G$1" pin="VDDFLASH" pad="95"/>
<connect gate="G$1" pin="VDDIN@1" pad="8"/>
<connect gate="G$1" pin="VDDIO@1" pad="17"/>
<connect gate="G$1" pin="VDDIO@2" pad="33"/>
<connect gate="G$1" pin="VDDIO@3" pad="48"/>
<connect gate="G$1" pin="VDDIO@4" pad="61"/>
<connect gate="G$1" pin="VDDIO@5" pad="84"/>
<connect gate="G$1" pin="VDDOUT@1" pad="7"/>
<connect gate="G$1" pin="VDDPLL" pad="100"/>
<connect gate="G$1" pin="XIN/PGMCK" pad="97"/>
<connect gate="G$1" pin="XOUT" pad="98"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT91SAM7X128B-AU"/>
<attribute name="OC_FARNELL" value="1288326"/>
<attribute name="OC_NEWARK" value="26R5682"/>
</technology>
<technology name="256">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT91SAM7X256B-AU"/>
<attribute name="OC_FARNELL" value="1288327"/>
<attribute name="OC_NEWARK" value="26R5683"/>
</technology>
<technology name="512">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT91SAM7X512-AU"/>
<attribute name="OC_FARNELL" value="1288328"/>
<attribute name="OC_NEWARK" value="23M5090"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT91SAM7X*-CU" prefix="IC">
<description>&lt;b&gt;Highly integrated Flash microcontrollers based on the 32-bit ARM RISC processor&lt;/b&gt;&lt;p&gt;
512/256/128 Kbyte high-speed Flash and 128/64/32 Kbyte SRAM, a large set of peripherals, including an 802.3 Ethernet MAC and a CAN controller&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/6120s.pdf</description>
<gates>
<gate name="G$1" symbol="AT91SAM7X-BGA"/>
</gates>
<devices>
<device name="" package="TFBGA100">
<connects>
<connect gate="G$1" pin="AD4" pad="K9"/>
<connect gate="G$1" pin="AD5" pad="K8"/>
<connect gate="G$1" pin="AD6" pad="K7"/>
<connect gate="G$1" pin="AD7" pad="K6"/>
<connect gate="G$1" pin="ADVREF" pad="K10"/>
<connect gate="G$1" pin="DDM" pad="K4"/>
<connect gate="G$1" pin="DDP" pad="K3"/>
<connect gate="G$1" pin="ERASE" pad="F7"/>
<connect gate="G$1" pin="GND@1" pad="E6"/>
<connect gate="G$1" pin="GND@2" pad="E10"/>
<connect gate="G$1" pin="GND@3" pad="F9"/>
<connect gate="G$1" pin="GND@4" pad="G8"/>
<connect gate="G$1" pin="GND@5" pad="J6"/>
<connect gate="G$1" pin="GND@6" pad="J9"/>
<connect gate="G$1" pin="GND@7" pad="K5"/>
<connect gate="G$1" pin="JTAGSEL" pad="H3"/>
<connect gate="G$1" pin="NRST" pad="D3"/>
<connect gate="G$1" pin="PA0/PGMEN0" pad="J3"/>
<connect gate="G$1" pin="PA1/PGMEN1" pad="J4"/>
<connect gate="G$1" pin="PA10/PGMM2" pad="D7"/>
<connect gate="G$1" pin="PA11/PGMM3" pad="D10"/>
<connect gate="G$1" pin="PA12/PGMD0" pad="C9"/>
<connect gate="G$1" pin="PA13/PGMD1" pad="C8"/>
<connect gate="G$1" pin="PA14/PGMD2" pad="B8"/>
<connect gate="G$1" pin="PA15/PGMD3" pad="C10"/>
<connect gate="G$1" pin="PA16/PGMD4" pad="B9"/>
<connect gate="G$1" pin="PA17/PGMD5" pad="B10"/>
<connect gate="G$1" pin="PA18/PGMD6" pad="A9"/>
<connect gate="G$1" pin="PA19/PGMD7" pad="B2"/>
<connect gate="G$1" pin="PA2" pad="G5"/>
<connect gate="G$1" pin="PA20/PGMD8" pad="A3"/>
<connect gate="G$1" pin="PA21/PGMD9" pad="A2"/>
<connect gate="G$1" pin="PA22/PGMD10" pad="A1"/>
<connect gate="G$1" pin="PA23/PGMD11" pad="D1"/>
<connect gate="G$1" pin="PA24/PGMD12" pad="D2"/>
<connect gate="G$1" pin="PA25/PGMD13" pad="E1"/>
<connect gate="G$1" pin="PA26/PGMD14" pad="E2"/>
<connect gate="G$1" pin="PA27/PGMD15" pad="G3"/>
<connect gate="G$1" pin="PA28" pad="H2"/>
<connect gate="G$1" pin="PA29" pad="J1"/>
<connect gate="G$1" pin="PA3" pad="H4"/>
<connect gate="G$1" pin="PA30" pad="J2"/>
<connect gate="G$1" pin="PA4/PGMNCMD" pad="H5"/>
<connect gate="G$1" pin="PA5/PGMRDY" pad="G6"/>
<connect gate="G$1" pin="PA6/PGMNOE" pad="F6"/>
<connect gate="G$1" pin="PA7/PGMNVALID" pad="H6"/>
<connect gate="G$1" pin="PA8/PGMM0" pad="H8"/>
<connect gate="G$1" pin="PA9/PGMM1" pad="H7"/>
<connect gate="G$1" pin="PB0" pad="C5"/>
<connect gate="G$1" pin="PB1" pad="A4"/>
<connect gate="G$1" pin="PB10" pad="C3"/>
<connect gate="G$1" pin="PB11" pad="B3"/>
<connect gate="G$1" pin="PB12" pad="B5"/>
<connect gate="G$1" pin="PB13" pad="C7"/>
<connect gate="G$1" pin="PB14" pad="B7"/>
<connect gate="G$1" pin="PB15" pad="B6"/>
<connect gate="G$1" pin="PB16" pad="C1"/>
<connect gate="G$1" pin="PB17" pad="C6"/>
<connect gate="G$1" pin="PB18" pad="E3"/>
<connect gate="G$1" pin="PB19" pad="D5"/>
<connect gate="G$1" pin="PB2" pad="B4"/>
<connect gate="G$1" pin="PB20" pad="E4"/>
<connect gate="G$1" pin="PB21" pad="F1"/>
<connect gate="G$1" pin="PB22" pad="G1"/>
<connect gate="G$1" pin="PB23" pad="F2"/>
<connect gate="G$1" pin="PB24" pad="G2"/>
<connect gate="G$1" pin="PB25" pad="F3"/>
<connect gate="G$1" pin="PB26" pad="F4"/>
<connect gate="G$1" pin="PB27/AD0" pad="D9"/>
<connect gate="G$1" pin="PB28/AD1" pad="E8"/>
<connect gate="G$1" pin="PB29/AD2" pad="H9"/>
<connect gate="G$1" pin="PB3" pad="C4"/>
<connect gate="G$1" pin="PB30/AD3" pad="G9"/>
<connect gate="G$1" pin="PB4" pad="C2"/>
<connect gate="G$1" pin="PB5" pad="A6"/>
<connect gate="G$1" pin="PB6" pad="D6"/>
<connect gate="G$1" pin="PB7" pad="A5"/>
<connect gate="G$1" pin="PB8" pad="A7"/>
<connect gate="G$1" pin="PB9" pad="A8"/>
<connect gate="G$1" pin="PLLRC" pad="H10"/>
<connect gate="G$1" pin="TCK" pad="F5"/>
<connect gate="G$1" pin="TDI" pad="B1"/>
<connect gate="G$1" pin="TDO" pad="G4"/>
<connect gate="G$1" pin="TMS" pad="E5"/>
<connect gate="G$1" pin="TST" pad="D4"/>
<connect gate="G$1" pin="VDDCORE@1" pad="F8"/>
<connect gate="G$1" pin="VDDCORE@2" pad="G7"/>
<connect gate="G$1" pin="VDDCORE@3" pad="H1"/>
<connect gate="G$1" pin="VDDCORE@4" pad="K1"/>
<connect gate="G$1" pin="VDDCORE@5" pad="K2"/>
<connect gate="G$1" pin="VDDFLASH" pad="J5"/>
<connect gate="G$1" pin="VDDIN@1" pad="F10"/>
<connect gate="G$1" pin="VDDIO@1" pad="A10"/>
<connect gate="G$1" pin="VDDIO@2" pad="D8"/>
<connect gate="G$1" pin="VDDIO@3" pad="E7"/>
<connect gate="G$1" pin="VDDIO@4" pad="E9"/>
<connect gate="G$1" pin="VDDOUT@1" pad="G10"/>
<connect gate="G$1" pin="VDDPLL" pad="J10"/>
<connect gate="G$1" pin="XIN/PGMCK" pad="J7"/>
<connect gate="G$1" pin="XOUT" pad="J8"/>
</connects>
<technologies>
<technology name="128">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="256">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT93C46A-10?Q-2.7" prefix="IC">
<description>&lt;b&gt;Three-wire Automotive Temperature Serial EEPROM&lt;/b&gt; 1K (64 x 16)&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc5089.pdf</description>
<gates>
<gate name="G$1" symbol="AT93C46A"/>
</gates>
<devices>
<device name="S" package="SOIC8">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DC" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT93C46DN-SH-B"/>
<attribute name="OC_FARNELL" value="1455086"/>
<attribute name="OC_NEWARK" value="58M3879"/>
</technology>
</technologies>
</device>
<device name="T" package="TSSOP8">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DC" pad="7"/>
<connect gate="G$1" pin="DI" pad="3"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="NC" pad="6"/>
<connect gate="G$1" pin="SK" pad="2"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY13" prefix="IC">
<description>&lt;b&gt; 8-bit AVR Microcontroller with 1K Bytes In-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
<gates>
<gate name="G$1" symbol="TINY13"/>
</gates>
<devices>
<device name="PU" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="5"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="6"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="7"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13-20PU"/>
<attribute name="OC_FARNELL" value="9171550"/>
<attribute name="OC_NEWARK" value="96K6521"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10PU"/>
<attribute name="OC_FARNELL" value="9171576"/>
<attribute name="OC_NEWARK" value="96K6523"/>
</technology>
</technologies>
</device>
<device name="SSU" package="8S1">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="5"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="6"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="7"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13-20SSU"/>
<attribute name="OC_FARNELL" value="1455133"/>
<attribute name="OC_NEWARK" value="58M3771"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10SSU"/>
<attribute name="OC_FARNELL" value="1455135"/>
<attribute name="OC_NEWARK" value="58M3773"/>
</technology>
</technologies>
</device>
<device name="SU" package="8S2">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="5"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="6"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="7"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="3"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13-20SU"/>
<attribute name="OC_FARNELL" value="9171568"/>
<attribute name="OC_NEWARK" value="96K6522"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10SU"/>
<attribute name="OC_FARNELL" value="9171584"/>
<attribute name="OC_NEWARK" value="96K6524"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TINY13*" prefix="IC">
<description>&lt;b&gt; 8-bit AVR Microcontroller with 1K Bytes In-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
<gates>
<gate name="G$1" symbol="TINY13"/>
<gate name="P" symbol="GND"/>
</gates>
<devices>
<device name="MM0" package="10M1">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="6"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="7"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="9"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="4"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="P" pin="GND" pad="11"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13A-MMU"/>
<attribute name="OC_FARNELL" value="1715516"/>
<attribute name="OC_NEWARK" value="15R0298"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13A-MMU"/>
<attribute name="OC_FARNELL" value="1715516"/>
<attribute name="OC_NEWARK" value="15R0298"/>
</technology>
</technologies>
</device>
<device name="MU" package="20M1">
<connects>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="PB0/PCINT0/AIN0/OC0A/MOSI" pad="11"/>
<connect gate="G$1" pin="PB1/PCINT1/AIN1/OC0B/INT0/MISO" pad="12"/>
<connect gate="G$1" pin="PB2/PCINT2/SCK/ADC1/T0" pad="14"/>
<connect gate="G$1" pin="PB3/PCINT3/CLKI/ADC3" pad="2"/>
<connect gate="G$1" pin="PB4/PCINT4/ADC2" pad="5"/>
<connect gate="G$1" pin="PB5/PCINT5/!RESET!/ADC0/DW" pad="1"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="P" pin="GND" pad="8"/>
</connects>
<technologies>
<technology name="-20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13A-MU"/>
<attribute name="OC_FARNELL" value="1715517"/>
<attribute name="OC_NEWARK" value="15R0299"/>
</technology>
<technology name="V-10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATTINY13V-10MU"/>
<attribute name="OC_FARNELL" value="1455134"/>
<attribute name="OC_NEWARK" value="58M3772"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="T7024" prefix="IC">
<description>&lt;b&gt;Bluetooth/ISM 2.4-GHz Front-End IC&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc4533.pdf</description>
<gates>
<gate name="G$1" symbol="T7024"/>
</gates>
<devices>
<device name="" package="MLF20-5X5-TH">
<connects>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="8"/>
<connect gate="G$1" pin="GND@3" pad="10"/>
<connect gate="G$1" pin="GND@4" pad="14"/>
<connect gate="G$1" pin="GND@5" pad="18"/>
<connect gate="G$1" pin="LNA_IN" pad="7"/>
<connect gate="G$1" pin="LNA_OUT" pad="1"/>
<connect gate="G$1" pin="PA_IN" pad="20"/>
<connect gate="G$1" pin="PU" pad="3"/>
<connect gate="G$1" pin="RAMP" pad="15"/>
<connect gate="G$1" pin="RX_ON" pad="2"/>
<connect gate="G$1" pin="R_SWITCH" pad="4"/>
<connect gate="G$1" pin="SWITCH_OUT" pad="5"/>
<connect gate="G$1" pin="V1_PA" pad="19"/>
<connect gate="G$1" pin="V2_PA@1" pad="16"/>
<connect gate="G$1" pin="V2_PA@2" pad="17"/>
<connect gate="G$1" pin="V3_PA_OUT@1" pad="11"/>
<connect gate="G$1" pin="V3_PA_OUT@2" pad="12"/>
<connect gate="G$1" pin="V3_PA_OUT@3" pad="13"/>
<connect gate="G$1" pin="VS_LNA" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA16A4" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;
&lt;h2&gt;Features&lt;/h2&gt;
&lt;ul&gt;&lt;li&gt; High-performance, Low-power 8/16-bit AVR XMEGA Microcontroller&lt;/li&gt;
&lt;li&gt; Non-Volatile Program and Data Memories&lt;/li&gt;
- 16 KB - 128 KB of In-System Self-Programmable Flash&lt;br&gt;
- 4 KB - 8 KB Boot Code Section with Independent Lock Bits&lt;br&gt;
- 1 KB - 2 KB EEPROM&lt;br&gt;
- 2 KB - 8 KB Internal SRAM
&lt;li&gt; Peripheral Features&lt;/li&gt;
- Four-channel DMA Controller with support for external requests&lt;br&gt;
- Eight-channel Event System&lt;br&gt;
- Five 16-bit Timer/Counters
&lt;ul&gt;Three Timer/Counters with 4 Output Compare or Input Capture channels&lt;/ul&gt;
&lt;ul&gt;Two Timer/Counters with 2 Output Compare or Input Capture channels&lt;/ul&gt;
&lt;ul&gt;High-Resolution Extensions on all Timer/Counters&lt;/ul&gt;
&lt;ul&gt;Advanced Waveform Extension on one Timer/Counter&lt;/ul&gt;
- Five USARTs
&lt;ul&gt;IrDA Extension on one USART&lt;/ul&gt;
- Two Two-Wire Interfaces with dual address match (I2C and SMBus compatible)&lt;br&gt;
- Two SPIs (Serial Peripheral Interfaces) peripherals&lt;br&gt;
- AES and DES Crypto Engine&lt;br&gt;
- 16-bit Real Time Counter with Separate Oscillator&lt;br&gt;
- One Twelve-channel, 12-bit, 2 Msps Analog to Digital Converter&lt;br&gt;
- One Two-channel, 12-bit, 1 Msps Digital to Analog Converter&lt;br&gt;
- Two Analog Comparators with Window compare function&lt;br&gt;
- External Interrupts on all General Purpose I/O pins&lt;br&gt;
- Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;li&gt; Special Microcontroller Features&lt;/li&gt;&lt;br&gt;
- Power-on Reset and Programmable Brown-out Detection&lt;br&gt;
- Internal and External Clock Options with PLL&lt;br&gt;
- Programmable Multi-level Interrupt Controller&lt;br&gt;
- Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby&lt;br&gt;
- Advanced Programming, Test and Debugging Interfaces
&lt;ul&gt;PDI (Program and Debug Interface) for programming, test and debugging&lt;/ul&gt;
&lt;li&gt; I/O and Packages&lt;/li&gt;
- 34 Programmable I/O Lines&lt;br&gt;
- 44 - lead TQFP&lt;br&gt;
- 44 - pad VQFN/QFN&lt;br&gt;
- 49 - ball VFBGA
&lt;li&gt; Operating Voltage&lt;/li&gt;
- 1.6 - 3.6V
&lt;li&gt; Speed performance&lt;/li&gt;
- 0 - 12 MHz @ 1.6 - 3.6V&lt;br&gt;
- 0 - 32 MHz @ 2.7 - 3.6V&lt;br&gt;&lt;/ul&gt;
&lt;p&gt;&lt;author&gt;Drawn by Dipl.-Ing. (FH) Robert Siegler&lt;/author&gt;&lt;/p&gt;
Created: 27.05.09</description>
<gates>
<gate name="G$1" symbol="XMEGA16A4"/>
</gates>
<devices>
<device name="A" package="TQFP44">
<connects>
<connect gate="G$1" pin="!RESET!/PDI_CLK" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="30"/>
<connect gate="G$1" pin="GND3" pad="38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI_DATA" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0(XT2)" pad="36"/>
<connect gate="G$1" pin="PR1(XT1)" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="19"/>
<connect gate="G$1" pin="VCC2" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="M1" package="MLF44-TH">
<connects>
<connect gate="G$1" pin="!RESET!/PDI_CLK" pad="35"/>
<connect gate="G$1" pin="AVCC" pad="39"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND1" pad="18"/>
<connect gate="G$1" pin="GND2" pad="30"/>
<connect gate="G$1" pin="GND3" pad="38"/>
<connect gate="G$1" pin="PA0" pad="40"/>
<connect gate="G$1" pin="PA1" pad="41"/>
<connect gate="G$1" pin="PA2" pad="42"/>
<connect gate="G$1" pin="PA3" pad="43"/>
<connect gate="G$1" pin="PA4" pad="44"/>
<connect gate="G$1" pin="PA5" pad="1"/>
<connect gate="G$1" pin="PA6" pad="2"/>
<connect gate="G$1" pin="PA7" pad="3"/>
<connect gate="G$1" pin="PB0" pad="4"/>
<connect gate="G$1" pin="PB1" pad="5"/>
<connect gate="G$1" pin="PB2" pad="6"/>
<connect gate="G$1" pin="PB3" pad="7"/>
<connect gate="G$1" pin="PC0" pad="10"/>
<connect gate="G$1" pin="PC1" pad="11"/>
<connect gate="G$1" pin="PC2" pad="12"/>
<connect gate="G$1" pin="PC3" pad="13"/>
<connect gate="G$1" pin="PC4" pad="14"/>
<connect gate="G$1" pin="PC5" pad="15"/>
<connect gate="G$1" pin="PC6" pad="16"/>
<connect gate="G$1" pin="PC7" pad="17"/>
<connect gate="G$1" pin="PD0" pad="20"/>
<connect gate="G$1" pin="PD1" pad="21"/>
<connect gate="G$1" pin="PD2" pad="22"/>
<connect gate="G$1" pin="PD3" pad="23"/>
<connect gate="G$1" pin="PD4" pad="24"/>
<connect gate="G$1" pin="PD5" pad="25"/>
<connect gate="G$1" pin="PD6" pad="26"/>
<connect gate="G$1" pin="PD7" pad="27"/>
<connect gate="G$1" pin="PDI_DATA" pad="34"/>
<connect gate="G$1" pin="PE0" pad="28"/>
<connect gate="G$1" pin="PE1" pad="29"/>
<connect gate="G$1" pin="PE2" pad="32"/>
<connect gate="G$1" pin="PE3" pad="33"/>
<connect gate="G$1" pin="PR0(XT2)" pad="36"/>
<connect gate="G$1" pin="PR1(XT1)" pad="37"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="19"/>
<connect gate="G$1" pin="VCC2" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XMEGA128A1" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;
&lt;h2&gt;Features&lt;/h2&gt;
&lt;ul&gt;&lt;li&gt;High-performance, Low-power 8/16-bit AVR XMEGA Microcontroller&lt;/li&gt;
&lt;li&gt; Non-Volatile Program and Data Memories&lt;/li&gt;
- 64K - 384K Bytes of In-System Self-Programmable Flash&lt;br&gt;
- 4K - 8K Bytes Boot Section with Independent Lock Bits&lt;br&gt;
- 2 KB - 4 KB EEPROM&lt;br&gt;
- 4 KB - 32 KB Internal SRAM
&lt;ul&gt;External Bus Interface for up to 16M bytes SRAM&lt;/ul&gt;
&lt;ul&gt;External Bus Interface for up to 128M bit SDRAM&lt;/ul&gt;
&lt;li&gt; Peripheral Features&lt;/li&gt;
- Four-channel DMA Controller with support for external requests&lt;br&gt;
- Eight-channel Event System&lt;br&gt;
- Eight 16-bit Timer/Counters
&lt;ul&gt;Four Timer/Counters with 4 Output Compare or Input Capture channels&lt;/ul&gt;
&lt;ul&gt;Four Timer/Counters with 2 Output Compare or Input Capture channels&lt;/ul&gt;
&lt;ul&gt;High-Resolution Extension on all Timer/Counters&lt;/ul&gt;
&lt;ul&gt;Advanced Waveform Extension on two Timer/Counters&lt;/ul&gt;
- Eight USARTs
&lt;ul&gt;IrDA modulation/demodulation for one USART&lt;/ul&gt;
- Four Two-Wire Interfaces with dual address match (I2C and SMBus compatible)&lt;br&gt;
- Four SPI (Serial Peripheral Interface) peripherals&lt;br&gt;
- AES and DES Crypto Engine&lt;br&gt;
- 16-bit Real Time Counter with separate Oscillator&lt;br&gt;
- Two Eight-channel, 12-bit, 2 Msps Analog to Digital Converters&lt;br&gt;
- Two Two-channel, 12-bit, 1 Msps Digital to Analog Converters&lt;br&gt;
- Four Analog Comparators with Window compare function&lt;br&gt;
- External Interrupts on all General Purpose I/O pins&lt;br&gt;
- Programmable Watchdog Timer with Separate On-chip Ultra Low Power Oscillator
&lt;li&gt; Special Microcontroller Features&lt;/li&gt;
- Power-on Reset and Programmable Brown-out Detection&lt;br&gt;
- Internal and External Clock Options with PLL and Prescaler&lt;br&gt;
- Programmable Multi-level Interrupt Controller&lt;br&gt;
- Sleep Modes: Idle, Power-down, Standby, Power-save, Extended Standby&lt;br&gt;
- Advanced Programming, Test and Debugging Interfaces
&lt;ul&gt;JTAG (IEEE 1149.1 Compliant) Interface for programming, test and debugging&lt;/ul&gt;
&lt;ul&gt;PDI (Program and Debug Interface) for programming and debugging&lt;/ul&gt;
&lt;li&gt; I/O and Packages&lt;/li&gt;
- 78 Programmable I/O Lines&lt;br&gt;
- 100 - lead TQFP&lt;br&gt;
- 100 - ball CBGA&lt;br&gt;
- 100 - ball VFBGA
&lt;li&gt; Operating Voltage&lt;/li&gt;
- 1.6 - 3.6V
&lt;li&gt; Speed performance&lt;/li&gt;
- 0 - 12 MHz @ 1.6 - 3.6V&lt;br&gt;
- 0 - 32 MHz @ 2.7 - 3.6V&lt;br&gt;&lt;/ul&gt;
&lt;p&gt;&lt;author&gt;Drawn by Dipl.-Ing. (FH) Robert Siegler&lt;/author&gt;&lt;/p&gt;
Created: 27.05.09</description>
<gates>
<gate name="G$1" symbol="XMEGA128A1"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G$1" pin="!RESET!/PDI_CLK" pad="90"/>
<connect gate="G$1" pin="AVCC" pad="4"/>
<connect gate="G$1" pin="AVCC1" pad="94"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND1" pad="13"/>
<connect gate="G$1" pin="GND2" pad="23"/>
<connect gate="G$1" pin="GND3" pad="33"/>
<connect gate="G$1" pin="GND4" pad="43"/>
<connect gate="G$1" pin="GND5" pad="53"/>
<connect gate="G$1" pin="GND6" pad="63"/>
<connect gate="G$1" pin="GND7" pad="73"/>
<connect gate="G$1" pin="GND8" pad="84"/>
<connect gate="G$1" pin="GND9" pad="93"/>
<connect gate="G$1" pin="PA0" pad="95"/>
<connect gate="G$1" pin="PA1" pad="96"/>
<connect gate="G$1" pin="PA2" pad="97"/>
<connect gate="G$1" pin="PA3" pad="98"/>
<connect gate="G$1" pin="PA4" pad="99"/>
<connect gate="G$1" pin="PA5" pad="100"/>
<connect gate="G$1" pin="PA6" pad="1"/>
<connect gate="G$1" pin="PA7" pad="2"/>
<connect gate="G$1" pin="PB0" pad="5"/>
<connect gate="G$1" pin="PB1" pad="6"/>
<connect gate="G$1" pin="PB2" pad="7"/>
<connect gate="G$1" pin="PB3" pad="8"/>
<connect gate="G$1" pin="PB4" pad="9"/>
<connect gate="G$1" pin="PB5" pad="10"/>
<connect gate="G$1" pin="PB6" pad="11"/>
<connect gate="G$1" pin="PB7" pad="12"/>
<connect gate="G$1" pin="PC0" pad="15"/>
<connect gate="G$1" pin="PC1" pad="16"/>
<connect gate="G$1" pin="PC2" pad="17"/>
<connect gate="G$1" pin="PC3" pad="18"/>
<connect gate="G$1" pin="PC4" pad="19"/>
<connect gate="G$1" pin="PC5" pad="20"/>
<connect gate="G$1" pin="PC6" pad="21"/>
<connect gate="G$1" pin="PC7" pad="22"/>
<connect gate="G$1" pin="PD0" pad="25"/>
<connect gate="G$1" pin="PD1" pad="26"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PDI_DATA" pad="89"/>
<connect gate="G$1" pin="PE0" pad="35"/>
<connect gate="G$1" pin="PE1" pad="36"/>
<connect gate="G$1" pin="PE2" pad="37"/>
<connect gate="G$1" pin="PE3" pad="38"/>
<connect gate="G$1" pin="PE4" pad="39"/>
<connect gate="G$1" pin="PE5" pad="40"/>
<connect gate="G$1" pin="PE6" pad="41"/>
<connect gate="G$1" pin="PE7" pad="42"/>
<connect gate="G$1" pin="PF0" pad="45"/>
<connect gate="G$1" pin="PF1" pad="46"/>
<connect gate="G$1" pin="PF2" pad="47"/>
<connect gate="G$1" pin="PF3" pad="48"/>
<connect gate="G$1" pin="PF4" pad="49"/>
<connect gate="G$1" pin="PF5" pad="50"/>
<connect gate="G$1" pin="PF6" pad="51"/>
<connect gate="G$1" pin="PF7" pad="52"/>
<connect gate="G$1" pin="PH0" pad="55"/>
<connect gate="G$1" pin="PH1" pad="56"/>
<connect gate="G$1" pin="PH2" pad="57"/>
<connect gate="G$1" pin="PH3" pad="58"/>
<connect gate="G$1" pin="PH4" pad="59"/>
<connect gate="G$1" pin="PH5" pad="60"/>
<connect gate="G$1" pin="PH6" pad="61"/>
<connect gate="G$1" pin="PH7" pad="62"/>
<connect gate="G$1" pin="PJ0" pad="65"/>
<connect gate="G$1" pin="PJ1" pad="66"/>
<connect gate="G$1" pin="PJ2" pad="67"/>
<connect gate="G$1" pin="PJ3" pad="68"/>
<connect gate="G$1" pin="PJ4" pad="69"/>
<connect gate="G$1" pin="PJ5" pad="70"/>
<connect gate="G$1" pin="PJ6" pad="71"/>
<connect gate="G$1" pin="PJ7" pad="72"/>
<connect gate="G$1" pin="PK0" pad="75"/>
<connect gate="G$1" pin="PK1" pad="76"/>
<connect gate="G$1" pin="PK2" pad="77"/>
<connect gate="G$1" pin="PK3" pad="78"/>
<connect gate="G$1" pin="PK4" pad="79"/>
<connect gate="G$1" pin="PK5" pad="80"/>
<connect gate="G$1" pin="PK6" pad="81"/>
<connect gate="G$1" pin="PK7" pad="82"/>
<connect gate="G$1" pin="PQ0" pad="85"/>
<connect gate="G$1" pin="PQ1" pad="86"/>
<connect gate="G$1" pin="PQ2" pad="87"/>
<connect gate="G$1" pin="PQ3" pad="88"/>
<connect gate="G$1" pin="PR0(XT2)" pad="91"/>
<connect gate="G$1" pin="PR1(XT1)" pad="92"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VCC1" pad="24"/>
<connect gate="G$1" pin="VCC2" pad="34"/>
<connect gate="G$1" pin="VCC3" pad="44"/>
<connect gate="G$1" pin="VCC4" pad="54"/>
<connect gate="G$1" pin="VCC5" pad="64"/>
<connect gate="G$1" pin="VCC6" pad="74"/>
<connect gate="G$1" pin="VCC7" pad="83"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA325P" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 32K Bytes In-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com .. doc8023.pdf</description>
<gates>
<gate name="G$1" symbol="ATMEGA325P"/>
</gates>
<devices>
<device name="" package="64M1">
<connects>
<connect gate="G$1" pin="!RESET!/PG5" pad="20"/>
<connect gate="G$1" pin="!SS!/PCINT8/PB0" pad="10"/>
<connect gate="G$1" pin="ADC0/PF0" pad="61"/>
<connect gate="G$1" pin="ADC1/PF1" pad="60"/>
<connect gate="G$1" pin="ADC2/PF2" pad="59"/>
<connect gate="G$1" pin="ADC3/PF3" pad="58"/>
<connect gate="G$1" pin="ADC4/TCK/PF4" pad="57"/>
<connect gate="G$1" pin="ADC5/TMS/PF5" pad="56"/>
<connect gate="G$1" pin="ADC6/TDO/PF6" pad="55"/>
<connect gate="G$1" pin="ADC7/TDI/PF7" pad="54"/>
<connect gate="G$1" pin="AIN1/PCINT3/PE3" pad="5"/>
<connect gate="G$1" pin="AREF" pad="62"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="CLKO/PCINT7/PE7" pad="9"/>
<connect gate="G$1" pin="DI/SDA/PCINT5/PE5" pad="7"/>
<connect gate="G$1" pin="DNC" pad="1"/>
<connect gate="G$1" pin="DO/PCINT6/PE6" pad="8"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="GND@1" pad="53"/>
<connect gate="G$1" pin="GND@2" pad="63"/>
<connect gate="G$1" pin="ICP1/PD0" pad="25"/>
<connect gate="G$1" pin="INT0/PD1" pad="26"/>
<connect gate="G$1" pin="MISO/PCINT11/PB3" pad="13"/>
<connect gate="G$1" pin="MOSI/PCINT10/PB2" pad="12"/>
<connect gate="G$1" pin="OC0A/PCINT12/PB4" pad="14"/>
<connect gate="G$1" pin="OC1A/PCINT13/PB5" pad="16"/>
<connect gate="G$1" pin="OC1B/PCINT14/PB6" pad="15"/>
<connect gate="G$1" pin="OC2A/PCINT15/PB7" pad="17"/>
<connect gate="G$1" pin="PA0" pad="51"/>
<connect gate="G$1" pin="PA1" pad="50"/>
<connect gate="G$1" pin="PA2" pad="49"/>
<connect gate="G$1" pin="PA3" pad="48"/>
<connect gate="G$1" pin="PA4" pad="47"/>
<connect gate="G$1" pin="PA5" pad="46"/>
<connect gate="G$1" pin="PA6" pad="45"/>
<connect gate="G$1" pin="PA7" pad="44"/>
<connect gate="G$1" pin="PC0" pad="35"/>
<connect gate="G$1" pin="PC1" pad="36"/>
<connect gate="G$1" pin="PC2" pad="37"/>
<connect gate="G$1" pin="PC3" pad="38"/>
<connect gate="G$1" pin="PC4" pad="39"/>
<connect gate="G$1" pin="PC5" pad="40"/>
<connect gate="G$1" pin="PC6" pad="41"/>
<connect gate="G$1" pin="PC7" pad="42"/>
<connect gate="G$1" pin="PD2" pad="27"/>
<connect gate="G$1" pin="PD3" pad="28"/>
<connect gate="G$1" pin="PD4" pad="29"/>
<connect gate="G$1" pin="PD5" pad="30"/>
<connect gate="G$1" pin="PD6" pad="31"/>
<connect gate="G$1" pin="PD7" pad="32"/>
<connect gate="G$1" pin="PG0" pad="33"/>
<connect gate="G$1" pin="PG1" pad="34"/>
<connect gate="G$1" pin="PG2" pad="43"/>
<connect gate="G$1" pin="RXD/PCINT0/PE0" pad="2"/>
<connect gate="G$1" pin="SCK/PCINT9/PB1" pad="11"/>
<connect gate="G$1" pin="T0/PG4" pad="19"/>
<connect gate="G$1" pin="T1/PG3" pad="18"/>
<connect gate="G$1" pin="TOSC1/XTAL1" pad="24"/>
<connect gate="G$1" pin="TOSC2/XTAL2" pad="23"/>
<connect gate="G$1" pin="TXD/PCINT1/PE1" pad="3"/>
<connect gate="G$1" pin="USCK/SCL/PCINT4/PE4" pad="6"/>
<connect gate="G$1" pin="VCC" pad="21"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="XCK/AIN0/PCINT2/PE2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA325PV-10AU"/>
<attribute name="OC_FARNELL" value="1636939"/>
<attribute name="OC_NEWARK" value="03P2025"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB642D" prefix="IC">
<description>&lt;b&gt;Flash-Memory 64-Megabit&lt;/b&gt; 2 .7-volt, Dual-interface, DataFlash&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc3542.pdf</description>
<gates>
<gate name="G$1" symbol="AT45DB642D"/>
</gates>
<devices>
<device name="" package="28T-TSOP-1">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="!RESET" pad="2"/>
<connect gate="G$1" pin="!WP" pad="3"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GNDP" pad="21"/>
<connect gate="G$1" pin="I/O0" pad="17"/>
<connect gate="G$1" pin="I/O1" pad="18"/>
<connect gate="G$1" pin="I/O2" pad="19"/>
<connect gate="G$1" pin="I/O3" pad="20"/>
<connect gate="G$1" pin="I/O4" pad="23"/>
<connect gate="G$1" pin="I/O5" pad="24"/>
<connect gate="G$1" pin="I/O6" pad="25"/>
<connect gate="G$1" pin="I/O7" pad="26"/>
<connect gate="G$1" pin="RDY/!BUSY" pad="1"/>
<connect gate="G$1" pin="SCK/CLK" pad="12"/>
<connect gate="G$1" pin="SER/!BYTE" pad="16"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="SO" pad="14"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VCCP" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AT45DB642D-TU"/>
<attribute name="OC_FARNELL" value="1095799"/>
<attribute name="OC_NEWARK" value="51P1801"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATMEGA644-*PU" prefix="IC">
<description>&lt;b&gt;8-bit Microcontroller with 64K Bytes In-System Programmable Flash&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc2593.pdf</description>
<gates>
<gate name="G$1" symbol="ATMEGA644-20PU"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!RESET" pad="9"/>
<connect gate="G$1" pin="AREF" pad="32"/>
<connect gate="G$1" pin="AVCC" pad="30"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="GND@1" pad="31"/>
<connect gate="G$1" pin="PCINT0/ADC0_PA0" pad="40"/>
<connect gate="G$1" pin="PCINT1/ADC1_PA1" pad="39"/>
<connect gate="G$1" pin="PCINT10/INT2/AIN0_PB2" pad="3"/>
<connect gate="G$1" pin="PCINT11/OC0A/AIN1_PB3" pad="4"/>
<connect gate="G$1" pin="PCINT12/OC0B/SS_PB4" pad="5"/>
<connect gate="G$1" pin="PCINT13/MOSI_PB5" pad="6"/>
<connect gate="G$1" pin="PCINT14/MISO_PB6" pad="7"/>
<connect gate="G$1" pin="PCINT15/SCK_PB7" pad="8"/>
<connect gate="G$1" pin="PCINT16/SCL_PC0" pad="22"/>
<connect gate="G$1" pin="PCINT17/SDA_PC1" pad="23"/>
<connect gate="G$1" pin="PCINT18/TCK_PC2" pad="24"/>
<connect gate="G$1" pin="PCINT19/TMS_PC3" pad="25"/>
<connect gate="G$1" pin="PCINT2/ADC2_PA2" pad="38"/>
<connect gate="G$1" pin="PCINT20/TDO_PC4" pad="26"/>
<connect gate="G$1" pin="PCINT21/TDI_PC5" pad="27"/>
<connect gate="G$1" pin="PCINT22/TOSC1_PC6" pad="28"/>
<connect gate="G$1" pin="PCINT23/TOSC2_PC7" pad="29"/>
<connect gate="G$1" pin="PCINT24/RXD0_PD0" pad="14"/>
<connect gate="G$1" pin="PCINT25/TXD0_PD1" pad="15"/>
<connect gate="G$1" pin="PCINT26/INT0_PD2" pad="16"/>
<connect gate="G$1" pin="PCINT27/INT1_PD3" pad="17"/>
<connect gate="G$1" pin="PCINT28/OC1B_PD4" pad="18"/>
<connect gate="G$1" pin="PCINT29/OC1A_PD5" pad="19"/>
<connect gate="G$1" pin="PCINT3/ADC3_PA3" pad="37"/>
<connect gate="G$1" pin="PCINT30/OC2B/ICP_PD6" pad="20"/>
<connect gate="G$1" pin="PCINT31/OC2A_PD7" pad="21"/>
<connect gate="G$1" pin="PCINT4/ADC4_PA4" pad="36"/>
<connect gate="G$1" pin="PCINT5/ADC5_PA5" pad="35"/>
<connect gate="G$1" pin="PCINT6/ADC6_PA6" pad="34"/>
<connect gate="G$1" pin="PCINT7/ADC7_PA7" pad="33"/>
<connect gate="G$1" pin="PCINT8/XCK0/T0_PB0" pad="1"/>
<connect gate="G$1" pin="PCINT9/CLKO/T1_PB1" pad="2"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
</connects>
<technologies>
<technology name="10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644V-10PU"/>
<attribute name="OC_FARNELL" value="1288342"/>
<attribute name="OC_NEWARK" value="23M5062"/>
</technology>
<technology name="20">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA644-20PU"/>
<attribute name="OC_FARNELL" value="1288340"/>
<attribute name="OC_NEWARK" value="23M5060"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AT45DB161D" prefix="IC">
<description>&lt;b&gt;16-megabit 2.5V or 2.7V DataFlash&lt;/b&gt;&lt;p&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/doc3500.pdf</description>
<gates>
<gate name="G$1" symbol="AT45DB161VFN8"/>
</gates>
<devices>
<device name="-MU" package="VDFN-8">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="!RESET" pad="3"/>
<connect gate="G$1" pin="!WP" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ATMEL"/>
<attribute name="MPN" value="AT45DB161D-SU"/>
<attribute name="OC_FARNELL" value="1455040"/>
</technology>
</technologies>
</device>
<device name="-SU" package="8S2">
<connects>
<connect gate="G$1" pin="!CS" pad="4"/>
<connect gate="G$1" pin="!RESET" pad="3"/>
<connect gate="G$1" pin="!WP" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="SCK" pad="2"/>
<connect gate="G$1" pin="SI" pad="1"/>
<connect gate="G$1" pin="SO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ATMEL"/>
<attribute name="MPN" value="AT45DB161D-SU"/>
<attribute name="OC_FARNELL" value="1455040"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
