<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="SO16-1">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO08-GW">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, gull wing</description>
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line&lt;/b&gt; 0.3 inch</description>
</package>
<package name="SO28-3">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL16/8">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="SO16-1/8">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO28-3/8">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL28">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL24/16">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="DIL24-4">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.4 inch</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line &lt;/b&gt; 0.3 inch</description>
</package>
<package name="D24-3/16">
<description>&lt;b&gt;Dual In Line&lt;/b&gt; 0.4 inch</description>
</package>
<package name="SSOP56DL">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP48DL">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="PLCC68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="SSOP28DL">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SOP08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="MSOP08">
<description>&lt;b&gt;Mini Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="SO20L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="SOP16">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO18L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
<package name="SO24L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;, large</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="TO220-7">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
<package name="DD-7">
<description>&lt;b&gt;DPAC&lt;b&gt;</description>
</package>
<package name="TO99">
<description>&lt;b&gt;Metal can Package&lt;/b&gt;</description>
</package>
<package name="SSOP20DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP24DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SOP20">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOJ28-4">
<description>&lt;b&gt;Small Outline J-Lead Package&lt;/b&gt;</description>
</package>
<package name="TSSOP024">
<description>&lt;b&gt;Thin Shrink Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP28BU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP24BU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP20BU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL14/7">
<description>&lt;b&gt;Dual In Line &lt;/b&gt;</description>
</package>
<package name="TO220-G5">
<description>&lt;b&gt;Molded Package&lt;/b&gt; TO-220 5 lead&lt;p&gt;
http://www.ti.com &lt;p&gt;
msot008b.pdf</description>
</package>
<package name="TO220-5">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
<package name="ZZ326">
<description>&lt;b&gt;Special Package&lt;/b&gt;</description>
</package>
<package name="SSOP16BU">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ml/msoi004e/msoi004e.pdf</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
<package name="DIL24/12">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO28-3/12">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DD-3">
<description>&lt;b&gt;DPAC&lt;/b&gt;</description>
</package>
<package name="PLCC28">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="PLCC-S28">
<description>&lt;b&gt;SOCKET&lt;/b&gt;&lt;p&gt;
Plastic leaded chip carrier, square</description>
</package>
<package name="DIL24-3/12">
<description>&lt;b&gt;Dual In Line&lt;/b&gt; 0.3 inch</description>
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
<package name="QSOP20">
<description>&lt;b&gt;Quarter-Size Small Outline Package&lt;/b&gt;</description>
</package>
<package name="TO220-5A">
<description>&lt;b&gt;Molded Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO16">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINES PACKAGE&lt;/b&gt; D (R-PDSO-G16)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ina2126.pdf</description>
</package>
<package name="TSSOP16-PW">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; PW (R-PDSO-G16)&lt;p&gt;

Source: www.ti.com .. ADS7828.pdf</description>
</package>
<package name="DW_RPDSO-G16">
<description>&lt;b&gt;DW (R-PDSO-G16)&lt;/b&gt;&lt;p&gt;
SOurce: http://focus.ti.com/lit/ds/symlink/ina217.pdf</description>
</package>
<package name="DB_R-PDSO-G28">
<description>&lt;b&gt;DB (R-PDSO-G28)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1210.pdf</description>
</package>
</packages>
<symbols>
<symbol name="INA2128">
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RGA" direction="pas"/>
<pin name="RGA@1" direction="pas"/>
<pin name="RGB" direction="pas"/>
<pin name="RGB@1" direction="pas"/>
<pin name="VOA" direction="out"/>
<pin name="VOB" direction="out"/>
<pin name="REFA" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="SENSEA" direction="in"/>
<pin name="SENSEB" direction="in"/>
</symbol>
<symbol name="INA2141">
<pin name="INA-" direction="in"/>
<pin name="INA+" direction="in"/>
<pin name="INB-" direction="in"/>
<pin name="INB+" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="JA" direction="pas"/>
<pin name="JA@1" direction="pas"/>
<pin name="JB" direction="pas"/>
<pin name="JB@1" direction="pas"/>
<pin name="VOA" direction="out"/>
<pin name="VOB" direction="out"/>
<pin name="REFA" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="SENSEA" direction="in"/>
<pin name="SENSEB" direction="in"/>
</symbol>
<symbol name="ISO130">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="VS1" direction="pwr"/>
<pin name="VS2" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
</symbol>
<symbol name="ADS7821">
<pin name="VIN" direction="in"/>
<pin name="BYTE" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13" direction="out"/>
<pin name="D14" direction="out"/>
<pin name="D15" direction="out"/>
<pin name="!BUSY" direction="out"/>
<pin name="REF"/>
<pin name="CAP" direction="pas"/>
<pin name="VANA" direction="pwr"/>
<pin name="VDIG" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="ADS7820">
<pin name="VIN" direction="in"/>
<pin name="BYTE" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="DZ@3" direction="pas"/>
<pin name="DZ@2" direction="pas"/>
<pin name="DZ@1" direction="pas"/>
<pin name="DZ" direction="pas"/>
<pin name="!BUSY" direction="out"/>
<pin name="REF"/>
<pin name="CAP" direction="pas"/>
<pin name="VANA" direction="pwr"/>
<pin name="VDIG" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="ADS7812">
<pin name="EXT/!INT" direction="in"/>
<pin name="!CONV" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="DATA" direction="out"/>
<pin name="!BUSY" direction="out"/>
<pin name="DATACLK"/>
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="R3IN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VS" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="BUF" direction="out"/>
<pin name="CAP" direction="pas"/>
<pin name="REF"/>
</symbol>
<symbol name="IVC102">
<pin name="IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="ISO122">
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="+VS1" direction="pwr"/>
<pin name="-VS1" direction="pwr"/>
<pin name="+VS2" direction="pwr"/>
<pin name="-VS2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="MPC506">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="IN9" direction="in"/>
<pin name="IN10" direction="in"/>
<pin name="IN11" direction="in"/>
<pin name="IN12" direction="in"/>
<pin name="IN13" direction="in"/>
<pin name="IN14" direction="in"/>
<pin name="IN15" direction="in"/>
<pin name="IN16" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="ENABLE" direction="in"/>
<pin name="VREF"/>
<pin name="+V" direction="pwr"/>
<pin name="-V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MPC507">
<pin name="IN1A" direction="in"/>
<pin name="IN2A" direction="in"/>
<pin name="IN3A" direction="in"/>
<pin name="IN4A" direction="in"/>
<pin name="IN5A" direction="in"/>
<pin name="IN6A" direction="in"/>
<pin name="IN7A" direction="in"/>
<pin name="IN8A" direction="in"/>
<pin name="IN1B" direction="in"/>
<pin name="IN2B" direction="in"/>
<pin name="IN3B" direction="in"/>
<pin name="IN4B" direction="in"/>
<pin name="IN5B" direction="in"/>
<pin name="IN6B" direction="in"/>
<pin name="IN7B" direction="in"/>
<pin name="IN8B" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="OUTB" direction="out"/>
<pin name="ENABLE" direction="in"/>
<pin name="VREF"/>
<pin name="+V" direction="pwr"/>
<pin name="-V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MPC508">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="-V" direction="pwr"/>
<pin name="+V" direction="pwr"/>
</symbol>
<symbol name="MPC509">
<pin name="IN1A" direction="in"/>
<pin name="IN2A" direction="in"/>
<pin name="IN3A" direction="in"/>
<pin name="IN4A" direction="in"/>
<pin name="IN1B" direction="in"/>
<pin name="IN2B" direction="in"/>
<pin name="IN3B" direction="in"/>
<pin name="IN4B" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="OUTB" direction="out"/>
<pin name="EN" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="-V" direction="pwr"/>
<pin name="+V" direction="pwr"/>
</symbol>
<symbol name="OPA124P">
<pin name="ON/CMP" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="ON" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="CMP" direction="pas"/>
<pin name="+VS" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
</symbol>
<symbol name="ISO164">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="A0" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="COM1/S1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="VS1+" direction="pwr"/>
<pin name="VS2+" direction="pwr"/>
<pin name="VS1-" direction="pwr"/>
<pin name="VS2-" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="ISO165">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="FBN" direction="pas"/>
<pin name="FBP" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="VS1+" direction="pwr"/>
<pin name="VS2+" direction="pwr"/>
<pin name="VS1-" direction="pwr"/>
<pin name="VS2-" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="ISO166">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="MOD" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
<pin name="+VS1" direction="pwr"/>
<pin name="+VS2" direction="pwr"/>
<pin name="-VS1" direction="pwr"/>
<pin name="-VS2" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="S1" direction="pas"/>
<pin name="S2" direction="pas"/>
</symbol>
<symbol name="AFE1115">
<pin name="TXDATA" direction="in"/>
<pin name="PLLIN" direction="in"/>
<pin name="TXSCLK" direction="in"/>
<pin name="TXCLK" direction="in"/>
<pin name="VCDATA" direction="in"/>
<pin name="VCSCLK" direction="in"/>
<pin name="VCLATCH" direction="in"/>
<pin name="RXSYNC" direction="in"/>
<pin name="RXLOOP" direction="in"/>
<pin name="RXGAIN0" direction="in"/>
<pin name="RXGAIN1" direction="in"/>
<pin name="RXLINE+" direction="in"/>
<pin name="RXLINE-" direction="in"/>
<pin name="RXHYB+" direction="in"/>
<pin name="RXHYB-" direction="in"/>
<pin name="VCINP" direction="in"/>
<pin name="RXD0" direction="out"/>
<pin name="RXD1" direction="out"/>
<pin name="RXD2" direction="out"/>
<pin name="RXD3" direction="out"/>
<pin name="RXD4" direction="out"/>
<pin name="RXD5" direction="out"/>
<pin name="RXD7" direction="out"/>
<pin name="RXD6" direction="out"/>
<pin name="RXD8" direction="out"/>
<pin name="RXD9" direction="out"/>
<pin name="RXD10" direction="out"/>
<pin name="RXD11" direction="out"/>
<pin name="RXD12" direction="out"/>
<pin name="RXD13" direction="out"/>
<pin name="PLLOUT" direction="out"/>
<pin name="VCM" direction="out"/>
<pin name="REFP" direction="out"/>
<pin name="REFN" direction="out"/>
<pin name="TXLINE+" direction="out"/>
<pin name="TXLINE-" direction="out"/>
<pin name="VCCLK" direction="out"/>
<pin name="VCOUT" direction="out"/>
<pin name="VCDAC" direction="out"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="GNDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AGND@5" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="AFE1104">
<pin name="PLLIN" direction="in"/>
<pin name="TXDAT" direction="in"/>
<pin name="TXCLK" direction="in"/>
<pin name="RXSYNC" direction="in"/>
<pin name="RXCLK" direction="in"/>
<pin name="RXLOOP" direction="in"/>
<pin name="RXGAIN0" direction="in"/>
<pin name="RXGAIN1" direction="in"/>
<pin name="RXHYBN" direction="in"/>
<pin name="RXHYBP" direction="in"/>
<pin name="RXLP" direction="in"/>
<pin name="RXLN" direction="in"/>
<pin name="PLLOUT" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13" direction="out"/>
<pin name="REFP" direction="out"/>
<pin name="REFN" direction="out"/>
<pin name="VCM" direction="out"/>
<pin name="LINEN" direction="out"/>
<pin name="LINEP" direction="out"/>
<pin name="PV" direction="pwr"/>
<pin name="DV" direction="pwr"/>
<pin name="AV" direction="pwr"/>
<pin name="AV@1" direction="pwr"/>
<pin name="AV@2" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
</symbol>
<symbol name="DAC4814">
<pin name="DATAIN" direction="in"/>
<pin name="!LATCHA" direction="in"/>
<pin name="!LATCHB" direction="in"/>
<pin name="!LATCHC" direction="in"/>
<pin name="!LATCHD" direction="in"/>
<pin name="INVIN" direction="in"/>
<pin name="BPOA" direction="in"/>
<pin name="BPOB" direction="in"/>
<pin name="BPOD" direction="in"/>
<pin name="BPOC" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!CLK" direction="in"/>
<pin name="DATAOUT" direction="out"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="INVOUT" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="+VL" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="AGND" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="DAC4815">
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="BPO" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!LE" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="REF-" direction="out"/>
<pin name="REF+" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="+VL" direction="pwr"/>
</symbol>
<symbol name="ADS7819">
<pin name="VIN" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="!BUSY" direction="out"/>
<pin name="CAP" direction="pas"/>
<pin name="+VANA" direction="pwr"/>
<pin name="+VANA@1" direction="pwr"/>
<pin name="-VANA" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="+VDIG@1" direction="pwr"/>
<pin name="+VDIG" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="REF"/>
<pin name="DGND@1" direction="pwr"/>
</symbol>
<symbol name="ADS7824">
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="PAR/!SER" direction="in"/>
<pin name="BYTE" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="CONTC" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="D0"/>
<pin name="D2"/>
<pin name="D4"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="D1" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="!BUSY" direction="out"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VS1" direction="pwr"/>
<pin name="VS2" direction="pwr"/>
<pin name="CAP" direction="in"/>
<pin name="REF"/>
</symbol>
<symbol name="ADS7833">
<pin name="V1-1N" direction="in"/>
<pin name="V1-1P" direction="in"/>
<pin name="V1-2N" direction="in"/>
<pin name="V1-2P" direction="in"/>
<pin name="V1-3N" direction="in"/>
<pin name="V1-3P" direction="in"/>
<pin name="V2-1N" direction="in"/>
<pin name="V2-1P" direction="in"/>
<pin name="V2-2N" direction="in"/>
<pin name="V2-2P" direction="in"/>
<pin name="V2-3N" direction="in"/>
<pin name="V2-3P" direction="in"/>
<pin name="V3-1N" direction="in"/>
<pin name="V3-1P" direction="in"/>
<pin name="V3-2N" direction="in"/>
<pin name="V3-2P" direction="in"/>
<pin name="V3-3N" direction="in"/>
<pin name="V3-3P" direction="in"/>
<pin name="V3-4N" direction="in"/>
<pin name="V3-4P" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SOUT1" direction="out"/>
<pin name="SOUT2" direction="out"/>
<pin name="SOUT3" direction="out"/>
<pin name="BUSY" direction="out"/>
<pin name="DCLOCK" direction="out"/>
<pin name="AOUT" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="NC@11" direction="nc"/>
<pin name="NC@12" direction="nc"/>
<pin name="NC@13" direction="nc"/>
<pin name="NC@14" direction="nc"/>
<pin name="NC@15" direction="nc"/>
<pin name="NC@16" direction="nc"/>
<pin name="NC@17" direction="nc"/>
<pin name="NC@18" direction="nc"/>
<pin name="NC@19" direction="nc"/>
<pin name="NC@20" direction="nc"/>
<pin name="NC@21" direction="nc"/>
<pin name="VANA+" direction="pwr"/>
<pin name="VANA-" direction="pwr"/>
<pin name="VDIG+" direction="pwr"/>
<pin name="VDIG-" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="SERIN" direction="in"/>
<pin name="ASH" direction="in"/>
<pin name="CONV" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="TP1" direction="pas"/>
<pin name="TP2" direction="pas"/>
<pin name="REFGND" direction="pwr"/>
<pin name="NC@22" direction="nc"/>
<pin name="NC@23" direction="nc"/>
<pin name="NC@24" direction="nc"/>
<pin name="NC@25" direction="nc"/>
<pin name="NC@26" direction="nc"/>
</symbol>
<symbol name="ADS800">
<pin name="IN" direction="in"/>
<pin name="!IN" direction="in"/>
<pin name="REFT" direction="pas"/>
<pin name="REFB" direction="pas"/>
<pin name="CM" direction="pas"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="MSBI" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="B10" direction="out"/>
<pin name="B11" direction="out"/>
<pin name="B12" direction="out"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="+VS@2" direction="pwr"/>
<pin name="+VS@3" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="ADS804">
<pin name="IN" direction="in"/>
<pin name="!IN" direction="in"/>
<pin name="REFT" direction="pas"/>
<pin name="REFB" direction="pas"/>
<pin name="CM" direction="pas"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="B10" direction="out"/>
<pin name="B11" direction="out"/>
<pin name="B12" direction="out"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="VDRV" direction="in"/>
<pin name="SEL" direction="in"/>
<pin name="OVR" direction="out"/>
</symbol>
<symbol name="ADS7817">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="DCLOCK" direction="in"/>
<pin name="!CS!/SHDN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="+VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ADS7806">
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="SB/!PTC" direction="in"/>
<pin name="EXT/!INT" direction="in"/>
<pin name="TAG" direction="in"/>
<pin name="BYTE" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="REFD" direction="in"/>
<pin name="DATACLK"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="SDATA" direction="out"/>
<pin name="!BUSY" direction="out"/>
<pin name="CAP" direction="pas"/>
<pin name="REF" direction="out"/>
<pin name="VANA" direction="pwr"/>
<pin name="VDIG" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="ADS7809">
<pin name="R1IN" direction="in"/>
<pin name="R2IN" direction="in"/>
<pin name="R3IN" direction="in"/>
<pin name="SB/!BTC" direction="in"/>
<pin name="EXT/!INT" direction="in"/>
<pin name="TAG" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="REF"/>
<pin name="DATACLK"/>
<pin name="DATA" direction="out"/>
<pin name="CAP" direction="pas"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="VDIG" direction="pwr"/>
<pin name="VANA" direction="pwr"/>
<pin name="SYNC" direction="out"/>
<pin name="!BUSY" direction="out"/>
</symbol>
<symbol name="ADS7815">
<pin name="VIN" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="!BUSY" direction="out"/>
<pin name="CAP" direction="pas"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="D13" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="D15" direction="pwr"/>
<pin name="D14" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="REF"/>
<pin name="D12" direction="pwr"/>
</symbol>
<symbol name="ADS1212">
<pin name="AINP" direction="in"/>
<pin name="AINN" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!DSYNC" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="VBIAS" direction="out"/>
<pin name="XOUT" direction="out"/>
<pin name="SDOUT" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!DRDY" direction="out"/>
</symbol>
<symbol name="ADS1213">
<pin name="AIN1P" direction="in"/>
<pin name="AIN1N" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!DSYNC" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="VBIAS" direction="out"/>
<pin name="XOUT" direction="out"/>
<pin name="SDOUT" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!DRDY" direction="out"/>
<pin name="AIN2P" direction="in"/>
<pin name="AIN2N" direction="in"/>
<pin name="AIN3P" direction="in"/>
<pin name="AIN3N" direction="in"/>
<pin name="AIN4P" direction="in"/>
<pin name="AIN4N" direction="in"/>
</symbol>
<symbol name="ADS1213E">
<pin name="AIN1P" direction="in"/>
<pin name="AIN1N" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!DSYNC" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="VBIAS" direction="out"/>
<pin name="XOUT" direction="out"/>
<pin name="SDOUT" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!DRDY" direction="out"/>
<pin name="AIN2P" direction="in"/>
<pin name="AIN2N" direction="in"/>
<pin name="AIN3P" direction="in"/>
<pin name="AIN3N" direction="in"/>
<pin name="AIN4P" direction="in"/>
<pin name="AIN4N" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
</symbol>
<symbol name="ADS1211">
<pin name="AIN1P" direction="in"/>
<pin name="AIN1N" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!DSYNC" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="VBIAS" direction="out"/>
<pin name="XOUT" direction="out"/>
<pin name="SDOUT" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!DRDY" direction="out"/>
<pin name="AIN2P" direction="in"/>
<pin name="AIN2N" direction="in"/>
<pin name="AIN3P" direction="in"/>
<pin name="AIN3N" direction="in"/>
<pin name="AIN4P" direction="in"/>
<pin name="AIN4N" direction="in"/>
</symbol>
<symbol name="ADS1211E">
<pin name="AIN1P" direction="in"/>
<pin name="AIN1N" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!DSYNC" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="VBIAS" direction="out"/>
<pin name="XOUT" direction="out"/>
<pin name="SDOUT" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="!DRDY" direction="out"/>
<pin name="AIN2P" direction="in"/>
<pin name="AIN2N" direction="in"/>
<pin name="AIN3P" direction="in"/>
<pin name="AIN3N" direction="in"/>
<pin name="AIN4P" direction="in"/>
<pin name="AIN4N" direction="in"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="ADS931">
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="+VS@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="REFT" direction="out"/>
<pin name="CM" direction="out"/>
<pin name="REFB" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="LPBY" direction="pas"/>
<pin name="LNBY" direction="pas"/>
<pin name="LVDD" direction="pwr"/>
</symbol>
<symbol name="ADS930">
<pin name="+IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="+VS@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="!IN" direction="in"/>
<pin name="CM" direction="out"/>
<pin name="1VREF" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="LPBY" direction="out"/>
<pin name="LNBY" direction="out"/>
<pin name="LVDD" direction="pwr"/>
</symbol>
<symbol name="ADS902">
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="+VS@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="REFT" direction="in"/>
<pin name="CM"/>
<pin name="REFB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="B10" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="LPBY" direction="pas"/>
<pin name="LNBY" direction="pas"/>
<pin name="LVDD" direction="pwr"/>
</symbol>
<symbol name="ADS900">
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="+VS@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="!IN" direction="in"/>
<pin name="CM" direction="out"/>
<pin name="1VREF" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="B10" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="LPBY" direction="out"/>
<pin name="LNBY" direction="out"/>
<pin name="LVDD" direction="pwr"/>
</symbol>
<symbol name="ADS801">
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="B12" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="+VS@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="!IN" direction="in"/>
<pin name="CM" direction="in"/>
<pin name="MSBI" direction="in"/>
<pin name="B11" direction="out"/>
<pin name="B10" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="REFT" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="+VS@3" direction="pwr"/>
</symbol>
<symbol name="ADS820">
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="MSBI" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="+VS@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="!IN" direction="in"/>
<pin name="CM" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="B10" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="REFT" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="+VS@3" direction="pwr"/>
</symbol>
<symbol name="ADS823">
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="INT/EXT" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="RSEL" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VDRV" direction="in"/>
<pin name="!IN" direction="in"/>
<pin name="CM" direction="in"/>
<pin name="PD" direction="in"/>
<pin name="BYB" direction="pas"/>
<pin name="B10" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="REFT" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="BYT" direction="pas"/>
</symbol>
<symbol name="2TRIMSUB">
<pin name="SUBS" direction="pas"/>
<pin name="TRIM1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="TRIM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="SUBS">
<pin name="SUBS" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="2TRIM">
<pin name="TRIM1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="TRIM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="2+2-">
<pin name="+VS2" direction="pwr"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="-VS2" direction="pwr"/>
<pin name="+VS1" direction="pwr"/>
<pin name="-VS1" direction="pwr"/>
</symbol>
<symbol name="OPA548">
<pin name="ILIM" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="E/S"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OP-AMP+-">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OP-AMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="2TRIMCAS">
<pin name="CASE" direction="pas"/>
<pin name="TRIM1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="TRIM2" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPA678">
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="CHA" direction="in"/>
<pin name="!CHA" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="+VCC" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="CCAP" direction="pas"/>
<pin name="COM" direction="pwr"/>
<pin name="DNC" direction="pas"/>
</symbol>
<symbol name="PCM1726">
<pin name="DIN" direction="in"/>
<pin name="SCKI" direction="in"/>
<pin name="FOR" direction="in"/>
<pin name="LRPL" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="ZERO" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="RES" direction="pas"/>
<pin name="CAP" direction="pas"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="TEST" direction="pas"/>
<pin name="RES@1" direction="pas"/>
</symbol>
<symbol name="PCM1727">
<pin name="DIN" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="ML" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="MD" direction="in"/>
<pin name="!RSTB" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="MCKO" direction="out"/>
<pin name="SCKO1" direction="out"/>
<pin name="SCKO2" direction="out"/>
<pin name="SCKO3" direction="out"/>
<pin name="XTO" direction="out"/>
<pin name="!ZERO" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VCA" direction="pwr"/>
<pin name="VCP" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="RSV" direction="pas"/>
<pin name="CAP" direction="pas"/>
</symbol>
<symbol name="PCM1725">
<pin name="DIN" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="DM" direction="in"/>
<pin name="SCKI" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="CAP" direction="pas"/>
<pin name="FOR" direction="in"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="PCM1723">
<pin name="DIN" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="ML" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="MD" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="MCKO" direction="out"/>
<pin name="SCKO" direction="out"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="XTO" direction="out"/>
<pin name="ZERO" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VCP" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="RES" direction="pas"/>
<pin name="CAP" direction="pas"/>
</symbol>
<symbol name="PCM1717">
<pin name="DIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="ML/MUTE" direction="in"/>
<pin name="MD/DM0" direction="in"/>
<pin name="MC/DM1" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="D/C_R" direction="out"/>
<pin name="D/C_L" direction="out"/>
<pin name="XTO" direction="out"/>
<pin name="ZERO" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="CLKO" direction="out"/>
</symbol>
<symbol name="PCM1715">
<pin name="DIN" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="MD" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="ML" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="EXT2R" direction="out"/>
<pin name="EXT2L" direction="out"/>
<pin name="EXT1R" direction="out"/>
<pin name="EXT1L" direction="out"/>
<pin name="XTO" direction="out"/>
<pin name="CLKO" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="OUTR" direction="out"/>
<pin name="CKSL" direction="in"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2R" direction="pwr"/>
<pin name="VCC2L" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2R" direction="pwr"/>
<pin name="AGND2L" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="RSTB" direction="in"/>
<pin name="VDD@1" direction="pwr"/>
</symbol>
<symbol name="PCM1721">
<pin name="SCKI" direction="in"/>
<pin name="ML" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="MD" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="MCKI" direction="in"/>
<pin name="SCKO" direction="out"/>
<pin name="ZERO" direction="out"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="RES" direction="pas"/>
<pin name="RES@1" direction="pas"/>
<pin name="CAP" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="PGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VCP" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="TEST" direction="pas"/>
</symbol>
<symbol name="PCM1720">
<pin name="DIN" direction="in"/>
<pin name="SCKI" direction="in"/>
<pin name="ML" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="MD" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="CAP" direction="pas"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="ZERO" direction="out"/>
<pin name="TEST" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="PCM1719">
<pin name="DIN" direction="in"/>
<pin name="PINR" direction="in"/>
<pin name="PINL" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="PMUTE" direction="in"/>
<pin name="MD" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="ML" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="POUTR" direction="out"/>
<pin name="POUTL" direction="out"/>
<pin name="XTO" direction="out"/>
<pin name="ZERO" direction="out"/>
<pin name="CLKO" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="PVCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="PAGND" direction="pwr"/>
<pin name="PCOM" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="COM" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="RSTB" direction="in"/>
</symbol>
<symbol name="PCM1718">
<pin name="DIN" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="FOR" direction="in"/>
<pin name="DM0" direction="in"/>
<pin name="DM1" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="XTO" direction="out"/>
<pin name="ZERO" direction="out"/>
<pin name="CLKO" direction="out"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="D/C_R" direction="pwr"/>
<pin name="D/C_L" direction="pwr"/>
</symbol>
<symbol name="PCM1702">
<pin name="DATA" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="IOUT" direction="out"/>
<pin name="+VCC" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="+VDD" direction="pwr"/>
<pin name="-VDD" direction="pwr"/>
<pin name="ACOM" direction="pwr"/>
<pin name="ACOM@1" direction="pwr"/>
<pin name="DCOM" direction="pwr"/>
<pin name="BPO" direction="pas"/>
<pin name="SERV" direction="pas"/>
<pin name="REF" direction="pas"/>
</symbol>
<symbol name="PCM1702U">
<pin name="DATA" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="IOUT" direction="out"/>
<pin name="+VCC" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="+VDD" direction="pwr"/>
<pin name="-VDD" direction="pwr"/>
<pin name="ACOM" direction="pwr"/>
<pin name="ACOM@1" direction="pwr"/>
<pin name="DCOM" direction="pwr"/>
<pin name="BPO" direction="pas"/>
<pin name="SERV" direction="pas"/>
<pin name="REF" direction="pas"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
</symbol>
<symbol name="PCM1710">
<pin name="DIN" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="MC/DM1" direction="in"/>
<pin name="MC/DM2" direction="in"/>
<pin name="ML/DSD" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="EXT2R" direction="out"/>
<pin name="EXT2L" direction="out"/>
<pin name="EXT1R" direction="out"/>
<pin name="EXT1L" direction="out"/>
<pin name="XTO" direction="out"/>
<pin name="CLKO" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="OUTR" direction="out"/>
<pin name="CKSL" direction="in"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2R" direction="pwr"/>
<pin name="VCC2L" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2R" direction="pwr"/>
<pin name="AGND2L" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="MUTE" direction="in"/>
<pin name="VDD@1" direction="pwr"/>
</symbol>
<symbol name="PCM1800">
<pin name="INR" direction="in"/>
<pin name="INL" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="BYPAS" direction="in"/>
<pin name="FMT0" direction="in"/>
<pin name="FMT1" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="SYSCLK" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="FSYNC"/>
<pin name="LRCK"/>
<pin name="BCK"/>
<pin name="VCC" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="CPL" direction="pas"/>
<pin name="CNL" direction="pas"/>
<pin name="CPR" direction="pas"/>
<pin name="CNR" direction="pas"/>
<pin name="REF2" direction="pas"/>
<pin name="REFCOM" direction="pas"/>
<pin name="REF1" direction="pas"/>
</symbol>
<symbol name="PCM3000">
<pin name="DIN" direction="in"/>
<pin name="INL" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="INR" direction="in"/>
<pin name="XTIN" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="MD" direction="in"/>
<pin name="ML" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="XTO" direction="out"/>
<pin name="CLKIO"/>
<pin name="REFL" direction="pas"/>
<pin name="REFR" direction="pas"/>
<pin name="CPR" direction="pas"/>
<pin name="CNR" direction="pas"/>
<pin name="CNL" direction="pas"/>
<pin name="CPL" direction="pas"/>
<pin name="VCOM" direction="pas"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
</symbol>
<symbol name="PCM3001">
<pin name="DIN" direction="in"/>
<pin name="INL" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="INR" direction="in"/>
<pin name="XTIN" direction="in"/>
<pin name="FMT2" direction="in"/>
<pin name="FMT1" direction="in"/>
<pin name="FMT0" direction="in"/>
<pin name="RSTB" direction="in"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="DOUT" direction="out"/>
<pin name="XTO" direction="out"/>
<pin name="CLKIO"/>
<pin name="REFL" direction="pas"/>
<pin name="REFR" direction="pas"/>
<pin name="CPR" direction="pas"/>
<pin name="CNR" direction="pas"/>
<pin name="CNL" direction="pas"/>
<pin name="CPL" direction="pas"/>
<pin name="VCOM" direction="pas"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
</symbol>
<symbol name="PCM1712">
<pin name="DIN" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="MC/DM1" direction="in"/>
<pin name="MC/DM2" direction="in"/>
<pin name="ML/DSD" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="EXT2R" direction="out"/>
<pin name="EXT2L" direction="out"/>
<pin name="EXT1R" direction="out"/>
<pin name="EXT1L" direction="out"/>
<pin name="XTO" direction="out"/>
<pin name="CLKO" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="OUTR" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2R" direction="pwr"/>
<pin name="VCC2L" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2R" direction="pwr"/>
<pin name="AGND2L" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="MUTE" direction="in"/>
<pin name="VDD@1" direction="pwr"/>
</symbol>
<symbol name="PGA206">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="VO1" direction="pas"/>
<pin name="VO2" direction="pas"/>
<pin name="VOS" direction="pas"/>
<pin name="VOS@1" direction="pas"/>
<pin name="SENSE" direction="pas"/>
<pin name="REF" direction="pas"/>
</symbol>
<symbol name="REF102">
<pin name="OUT" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="TRIM" direction="pas"/>
<pin name="NR" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="COM" direction="pwr"/>
</symbol>
<symbol name="REF200">
<pin name="MIN" direction="in"/>
<pin name="MOUT" direction="out"/>
<pin name="I1H" direction="pas"/>
<pin name="I2H" direction="pas"/>
<pin name="I1L" direction="pas"/>
<pin name="I2L" direction="pas"/>
<pin name="MCOM" direction="pas"/>
<pin name="SUBST" direction="pas"/>
</symbol>
<symbol name="REF1004">
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="C1" direction="pas"/>
</symbol>
<symbol name="XTR101">
<pin name="OUT" direction="out"/>
<pin name="REF1" direction="out"/>
<pin name="REF2" direction="out"/>
<pin name="BCONT" direction="out"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="ZA" direction="pas"/>
<pin name="ZA@1" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="ZA@2" direction="pwr"/>
<pin name="SPAN" direction="pwr"/>
<pin name="SPAN@1" direction="pwr"/>
<pin name="E" direction="pas"/>
<pin name="BW" direction="pas"/>
</symbol>
<symbol name="XTR101U">
<pin name="OUT" direction="out"/>
<pin name="REF1" direction="out"/>
<pin name="REF2" direction="out"/>
<pin name="BCONT" direction="out"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="ZA" direction="pas"/>
<pin name="ZA@1" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="ZA@2" direction="pwr"/>
<pin name="SPAN" direction="pwr"/>
<pin name="SPAN@1" direction="pwr"/>
<pin name="E" direction="pas"/>
<pin name="BW" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="DAC712">
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="D12" direction="in"/>
<pin name="D13" direction="in"/>
<pin name="D14" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="DCOM" direction="pwr"/>
<pin name="ACOM" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="+VCC" direction="pwr"/>
<pin name="OA" direction="pas"/>
<pin name="GA" direction="pas"/>
<pin name="D15" direction="in"/>
</symbol>
<symbol name="DAC714">
<pin name="SDI" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!CLK" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="FB2" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="BPO" direction="pas"/>
<pin name="OA" direction="pas"/>
<pin name="GA" direction="pas"/>
<pin name="DCOM" direction="pwr"/>
<pin name="ACOM" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="+VCC" direction="pwr"/>
</symbol>
<symbol name="DAC725">
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="!A0" direction="in"/>
<pin name="!A1" direction="in"/>
<pin name="!A2" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!WRA" direction="in"/>
<pin name="!WRB" direction="in"/>
<pin name="!CSA" direction="in"/>
<pin name="!CSB" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="DCOM" direction="pwr"/>
<pin name="ACOMB" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="+VCC" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="ACOMA" direction="pwr"/>
<pin name="SJA" direction="pas"/>
<pin name="SJB" direction="pas"/>
<pin name="GAB" direction="pas"/>
<pin name="GAA" direction="pas"/>
</symbol>
<symbol name="DAC813">
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!LDAC" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="!LMSB" direction="in"/>
<pin name="!LLSB" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="BPO" direction="pas"/>
<pin name="RANGE" direction="pas"/>
<pin name="DCOM" direction="pwr"/>
<pin name="REFOUT" direction="out"/>
<pin name="ACOM" direction="pwr"/>
<pin name="+VL" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="+VCC" direction="pwr"/>
<pin name="RANGE@1" direction="pas"/>
</symbol>
<symbol name="DAC4813">
<pin name="DB0" direction="in"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="DB8" direction="in"/>
<pin name="DB9" direction="in"/>
<pin name="DB10" direction="in"/>
<pin name="DB11" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="EN3" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!LDAC" direction="in"/>
<pin name="EN4" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="DCOM" direction="pwr"/>
<pin name="ACOM" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="+VCC" direction="pwr"/>
</symbol>
<symbol name="DAC7800">
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!UPDA" direction="in"/>
<pin name="!UPDB" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGNDA" direction="pwr"/>
<pin name="AGNDB" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="REFA" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="FBA" direction="pas"/>
<pin name="FBB" direction="pas"/>
</symbol>
<symbol name="DAC7801">
<pin name="DB0" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!UPD" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGNDA" direction="pwr"/>
<pin name="AGNDB" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="REFA" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="FBA" direction="pas"/>
<pin name="FBB" direction="pas"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
</symbol>
<symbol name="DAC7802">
<pin name="DB0" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!CSA" direction="in"/>
<pin name="DB9" direction="in"/>
<pin name="DB8" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="!CSB" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="REFA" direction="in"/>
<pin name="REFB" direction="in"/>
<pin name="FBA" direction="pas"/>
<pin name="FBB" direction="pas"/>
<pin name="DB1" direction="in"/>
<pin name="DB2" direction="in"/>
<pin name="DB3" direction="in"/>
<pin name="DB4" direction="in"/>
<pin name="DB5" direction="in"/>
<pin name="DB6" direction="in"/>
<pin name="DB7" direction="in"/>
<pin name="DB10" direction="in"/>
<pin name="DB11" direction="in"/>
</symbol>
<symbol name="INA141">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="J" direction="pas"/>
<pin name="J@1" direction="pas"/>
<pin name="REF" direction="pas"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="DCP0124">
<pin name="SYIN" direction="in"/>
<pin name="SYOUT" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="+VOUT" direction="pwr"/>
<pin name="0V" direction="pwr"/>
<pin name="0V@1" direction="pwr"/>
</symbol>
<symbol name="DCP0124D">
<pin name="SYIN" direction="in"/>
<pin name="SYOUT" direction="out"/>
<pin name="-VOUT" direction="nc"/>
<pin name="VS" direction="pwr"/>
<pin name="+VOUT" direction="pwr"/>
<pin name="0V" direction="pwr"/>
<pin name="0V@1" direction="pwr"/>
</symbol>
<symbol name="XTR103">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="ZA" direction="pas"/>
<pin name="ZA@1" direction="pas"/>
<pin name="ZA@2" direction="pas"/>
<pin name="RG" direction="pas"/>
<pin name="RG@1" direction="pas"/>
<pin name="B" direction="out"/>
<pin name="E" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="RLIN" direction="pas"/>
<pin name="RLIN@1" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="IR2" direction="pas"/>
<pin name="IR1" direction="pas"/>
<pin name="EINT" direction="pas"/>
</symbol>
<symbol name="XTR104">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="ZA" direction="pas"/>
<pin name="ZA@1" direction="pas"/>
<pin name="ZA@2" direction="pas"/>
<pin name="RG" direction="pas"/>
<pin name="RG@1" direction="pas"/>
<pin name="B" direction="out"/>
<pin name="E" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="+LIN" direction="in"/>
<pin name="-LIN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="RLIN@1" direction="pas"/>
<pin name="VREF" direction="out"/>
<pin name="RLIN" direction="pas"/>
</symbol>
<symbol name="XTR105">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="VLIN" direction="pas"/>
<pin name="VREG" direction="out"/>
<pin name="RG" direction="pas"/>
<pin name="RG@1" direction="pas"/>
<pin name="B" direction="out"/>
<pin name="E" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="OUT" direction="out"/>
<pin name="IR2" direction="pas"/>
<pin name="IR1" direction="pas"/>
<pin name="IRET" direction="in"/>
</symbol>
<symbol name="ADS901">
<pin name="IN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="+VS@1" direction="pwr"/>
<pin name="+VS@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="REFT" direction="in"/>
<pin name="CM" direction="out"/>
<pin name="REFB" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="B10" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="LPBY" direction="pas"/>
<pin name="LNBY" direction="pas"/>
<pin name="LVDD" direction="pwr"/>
</symbol>
<symbol name="ADS574">
<pin name="DB0" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB7" direction="out"/>
<pin name="DB8" direction="out"/>
<pin name="DB9" direction="out"/>
<pin name="DB10" direction="out"/>
<pin name="DB11" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="CE" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="BO" direction="in"/>
<pin name="10VR" direction="in"/>
<pin name="20VR" direction="in"/>
<pin name="STATUS" direction="out"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="AO" direction="in"/>
<pin name="12/!8" direction="in"/>
<pin name="REFOUT" direction="out"/>
<pin name="VEE" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="ACOM" direction="pwr"/>
<pin name="DCOM" direction="pwr"/>
</symbol>
<symbol name="ADS7800">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="HBE" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="!BUSY" direction="out"/>
<pin name="VSA" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VSD" direction="pwr"/>
</symbol>
<symbol name="ACF2101">
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="RESA" direction="in"/>
<pin name="RESB" direction="in"/>
<pin name="HOLDA" direction="in"/>
<pin name="HOLDB" direction="in"/>
<pin name="SELA" direction="in"/>
<pin name="SELB" direction="in"/>
<pin name="GNDA" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="COMA" direction="in"/>
<pin name="COMB" direction="in"/>
<pin name="SCOMA" direction="out"/>
<pin name="SCOMB" direction="out"/>
<pin name="CAPA" direction="pas"/>
<pin name="CAPB" direction="pas"/>
<pin name="SINA" direction="in"/>
<pin name="SINB" direction="in"/>
<pin name="SOUTA" direction="out"/>
<pin name="SOUTB" direction="out"/>
<pin name="GNDB" direction="pwr"/>
</symbol>
<symbol name="AFE1103">
<pin name="PLLIN" direction="in"/>
<pin name="TXDP" direction="in"/>
<pin name="TXDN" direction="in"/>
<pin name="TXCLK" direction="in"/>
<pin name="RXSYNC" direction="in"/>
<pin name="RXLOOP" direction="in"/>
<pin name="RXGAIN0" direction="in"/>
<pin name="RXGAIN1" direction="in"/>
<pin name="RXLP" direction="in"/>
<pin name="RXLN" direction="in"/>
<pin name="RXHYBP" direction="in"/>
<pin name="RXHYBN" direction="in"/>
<pin name="RXD0" direction="out"/>
<pin name="RXD1" direction="out"/>
<pin name="RXD2" direction="out"/>
<pin name="RXD3" direction="out"/>
<pin name="RXD4" direction="out"/>
<pin name="RXD5" direction="out"/>
<pin name="RXD6" direction="out"/>
<pin name="RXD7" direction="out"/>
<pin name="RXD8" direction="out"/>
<pin name="RXD9" direction="out"/>
<pin name="RXD10" direction="out"/>
<pin name="RXD11" direction="out"/>
<pin name="RXD12" direction="out"/>
<pin name="RXD13" direction="out"/>
<pin name="PLLOUT" direction="out"/>
<pin name="TXLP" direction="out"/>
<pin name="REFP" direction="out"/>
<pin name="TXLN" direction="out"/>
<pin name="VCM" direction="out"/>
<pin name="REFN" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="PVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="AVDD@2" direction="pwr"/>
</symbol>
<symbol name="DDC101U">
<pin name="DIN" direction="in"/>
<pin name="!RESYS" direction="in"/>
<pin name="!FDS" direction="in"/>
<pin name="SYSCLK" direction="in"/>
<pin name="DATACLK" direction="in"/>
<pin name="DATAIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="!DVAL" direction="out"/>
<pin name="!OVF+" direction="out"/>
<pin name="!OVF-" direction="out"/>
<pin name="!DTR" direction="in"/>
<pin name="RD/!SE" direction="in"/>
<pin name="!RESE" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="REFBB" direction="pas"/>
<pin name="DGND" direction="nc"/>
<pin name="SETUP" direction="in"/>
<pin name="VS+" direction="pwr"/>
<pin name="VS+@1" direction="pwr"/>
<pin name="VS-" direction="pwr"/>
<pin name="VDD+" direction="pwr"/>
<pin name="ANACOM" direction="pwr"/>
<pin name="ANACOM@1" direction="pwr"/>
</symbol>
<symbol name="DDC101P">
<pin name="DIN" direction="in"/>
<pin name="!RESYS" direction="in"/>
<pin name="!FDS" direction="in"/>
<pin name="SYSCLK" direction="in"/>
<pin name="DATACLK" direction="in"/>
<pin name="DATAIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="!DVAL" direction="out"/>
<pin name="!OVF+" direction="out"/>
<pin name="!OVF-" direction="out"/>
<pin name="!DTR" direction="in"/>
<pin name="RD/!SE" direction="in"/>
<pin name="!RESE" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="REFBB" direction="pas"/>
<pin name="DGND" direction="nc"/>
<pin name="SETUP" direction="in"/>
<pin name="VS+" direction="pwr"/>
<pin name="VS+@1" direction="pwr"/>
<pin name="VS-" direction="pwr"/>
<pin name="VDD+" direction="pwr"/>
<pin name="ANACOM" direction="pwr"/>
<pin name="ANACOM@1" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
</symbol>
<symbol name="PCM63P">
<pin name="DATA" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="NC@4" direction="nc"/>
<pin name="BPO" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC" direction="nc"/>
<pin name="SCAP" direction="pas"/>
<pin name="RCAP" direction="pas"/>
<pin name="OCAP" direction="pas"/>
<pin name="RF1" direction="pas"/>
<pin name="RF2" direction="pas"/>
<pin name="UB2" direction="pas"/>
<pin name="LB2" direction="pas"/>
<pin name="POT" direction="pas"/>
<pin name="ACOM" direction="pwr"/>
<pin name="-VD" direction="pwr"/>
<pin name="+VD" direction="pwr"/>
<pin name="-VA" direction="pwr"/>
<pin name="+VA" direction="pwr"/>
<pin name="DCOM" direction="pwr"/>
</symbol>
<symbol name="INA128">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="REF" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG" direction="pas"/>
<pin name="RG@1" direction="pas"/>
</symbol>
<symbol name="INA134">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="SENSE" direction="pas"/>
<pin name="REF" direction="pas"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="INA2134">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="SENSEA" direction="pas"/>
<pin name="REFA" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="OUTB" direction="out"/>
<pin name="SENSEB" direction="pas"/>
<pin name="REFB" direction="pas"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="INA122">
<pin name="+IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG@1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="REF" direction="pas"/>
</symbol>
<symbol name="INA118">
<pin name="-IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG@1" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="REF" direction="pas"/>
</symbol>
<symbol name="INA125">
<pin name="+IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG@1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="REFOUT" direction="out"/>
<pin name="REF10" direction="out"/>
<pin name="REF5" direction="out"/>
<pin name="REF2.5" direction="out"/>
<pin name="REFBG" direction="out"/>
<pin name="REFCOM" direction="pas"/>
<pin name="!SLEEP" direction="in"/>
<pin name="SENSE" direction="pas"/>
</symbol>
<symbol name="INA117">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="COMP" direction="pas"/>
<pin name="REFA" direction="in"/>
<pin name="REFB" direction="in"/>
</symbol>
<symbol name="INA116">
<pin name="-IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG@1" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="GUARD-" direction="pas"/>
<pin name="GUARD-@1" direction="pas"/>
<pin name="GUARD+" direction="pas"/>
<pin name="GUARD+@1" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
</symbol>
<symbol name="INA114">
<pin name="-IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG@1" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="REF" direction="pas"/>
</symbol>
<symbol name="INA114U">
<pin name="-IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG@1" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="INA103">
<pin name="-IN" direction="in"/>
<pin name="-GS" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="+GS" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="G=100" direction="pas"/>
<pin name="+RG" direction="pas"/>
<pin name="SENSE" direction="in"/>
<pin name="-RG" direction="pas"/>
<pin name="-GD" direction="pas"/>
<pin name="+GD" direction="pas"/>
<pin name="+OFFS" direction="pas"/>
<pin name="-OFFS" direction="pas"/>
</symbol>
<symbol name="INA2126">
<pin name="+INA" direction="in"/>
<pin name="-INA" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="SENSEA" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="SENSEB" direction="pas"/>
<pin name="RGA" direction="pas"/>
<pin name="RGA@1" direction="pas"/>
<pin name="RGB" direction="pas"/>
<pin name="RGB@1" direction="pas"/>
<pin name="REFA" direction="pwr"/>
<pin name="REFB" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="INA126">
<pin name="+IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG@1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="REF" direction="pas"/>
</symbol>
<symbol name="ISO212">
<pin name="+I/P" direction="in"/>
<pin name="-I/P" direction="in"/>
<pin name="CLKIN" direction="in"/>
<pin name="O/PHIGH" direction="out"/>
<pin name="O/PLOW" direction="out"/>
<pin name="CLKOUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="COM1" direction="pwr"/>
<pin name="COM2" direction="pwr"/>
<pin name="OFFA" direction="pas"/>
<pin name="OFFA@1" direction="pas"/>
<pin name="+VSS1" direction="out"/>
<pin name="-VSS1" direction="out"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="BUF634">
<pin name="BW" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="BUF634P">
<pin name="BW" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
</symbol>
<symbol name="DAC56">
<pin name="DATA" direction="in"/>
<pin name="LE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="LCOM" direction="pwr"/>
<pin name="ACOM" direction="pwr"/>
<pin name="-VS" direction="pwr"/>
<pin name="+VS" direction="pwr"/>
<pin name="-VL" direction="pwr"/>
<pin name="+VL" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="TRIM" direction="pas"/>
<pin name="RF" direction="pas"/>
<pin name="SJ" direction="pas"/>
<pin name="MSBAD" direction="pas"/>
</symbol>
<symbol name="REG1118">
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ISO124">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND2" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="-VS2" direction="pwr"/>
<pin name="+VS2" direction="pwr"/>
<pin name="-VS1" direction="pwr"/>
<pin name="+VS1" direction="pwr"/>
</symbol>
<symbol name="ISO150">
<pin name="D1A"/>
<pin name="D1B"/>
<pin name="D2B"/>
<pin name="D2A"/>
<pin name="R/!T1A" direction="in"/>
<pin name="R/!T2A" direction="in"/>
<pin name="R/!T1B" direction="in"/>
<pin name="R/!T2B" direction="in"/>
<pin name="GB" direction="pwr"/>
<pin name="GA" direction="pwr"/>
<pin name="VSA" direction="pwr"/>
<pin name="VSB" direction="pwr"/>
</symbol>
<symbol name="ADS7804">
<pin name="IN" direction="in"/>
<pin name="BYTE" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="B0" direction="out"/>
<pin name="B1" direction="out"/>
<pin name="B2" direction="out"/>
<pin name="B3" direction="out"/>
<pin name="B4" direction="out"/>
<pin name="B5" direction="out"/>
<pin name="B6" direction="out"/>
<pin name="B7" direction="out"/>
<pin name="B8" direction="out"/>
<pin name="B9" direction="out"/>
<pin name="B10" direction="out"/>
<pin name="B11" direction="out"/>
<pin name="B12" direction="out"/>
<pin name="B13" direction="out"/>
<pin name="B14" direction="out"/>
<pin name="B15" direction="out"/>
<pin name="VANA" direction="pwr"/>
<pin name="VDIG" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="REF"/>
<pin name="CAP" direction="pas"/>
<pin name="!BUSY" direction="out"/>
</symbol>
<symbol name="ADS7803">
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="/WR" direction="in"/>
<pin name="/RD" direction="in"/>
<pin name="/CS" direction="in"/>
<pin name="/BUSY" direction="in"/>
<pin name="HBE" direction="in"/>
<pin name="/CAL" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="SFR" direction="in"/>
<pin name="VREF+"/>
<pin name="VREF-"/>
<pin name="VD"/>
</symbol>
<symbol name="DAC7541A">
<pin name="B1(MSB)" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="B8" direction="in"/>
<pin name="B9" direction="in"/>
<pin name="B10" direction="in"/>
<pin name="B11" direction="in"/>
<pin name="B12(LSB)" direction="in"/>
<pin name="IOUT1" direction="out"/>
<pin name="IOUT2" direction="out"/>
<pin name="VREF" direction="pwr"/>
<pin name="FEEDBACK" direction="pas"/>
</symbol>
<symbol name="XTR110A">
<pin name="V_FORCE" direction="pas"/>
<pin name="V_SENSE" direction="pas"/>
<pin name="V_ADJUST" direction="pas"/>
<pin name="VIN(10)" direction="pas"/>
<pin name="VREF_IN" direction="pas"/>
<pin name="VIN(5V)" direction="pas"/>
<pin name="SRES" direction="pas"/>
<pin name="SSENSE" direction="pas"/>
<pin name="GATE" direction="pas"/>
<pin name="OFFSET1" direction="pas"/>
<pin name="OFFSET2" direction="pas"/>
<pin name="SPAN" direction="pas"/>
<pin name="4MASPAN" direction="pas"/>
<pin name="16MASPAN" direction="pas"/>
</symbol>
<symbol name="PWR+-12V">
<pin name="+12V" direction="pwr"/>
<pin name="-12V" direction="pwr"/>
</symbol>
<symbol name="2101BP">
<pin name="OUTA" direction="out"/>
<pin name="GNDA" direction="pas"/>
<pin name="COMA" direction="in"/>
<pin name="CAPA" direction="pas"/>
<pin name="INA" direction="in"/>
<pin name="SWINA" direction="in"/>
<pin name="SWINB" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="CAPB" direction="pas"/>
<pin name="COMB" direction="pas"/>
<pin name="GNDB" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="SWOUTB" direction="out"/>
<pin name="SWCOMB" direction="pas"/>
<pin name="SELECTB" direction="pas"/>
<pin name="RESETB" direction="pas"/>
<pin name="HOLDB" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="HOLDA" direction="pas"/>
<pin name="RESETA" direction="pas"/>
<pin name="SELECTA" direction="pas"/>
<pin name="SWCOMA" direction="pas"/>
<pin name="SWOUTA" direction="pas"/>
</symbol>
<symbol name="2101BU">
<pin name="SWINB" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="CAPB" direction="pas"/>
<pin name="COMB" direction="pas"/>
<pin name="GNDB" direction="pas"/>
<pin name="OUTB" direction="out"/>
<pin name="SWOUTB" direction="out"/>
<pin name="SWCOMB" direction="pas"/>
<pin name="SELECTB" direction="pas"/>
<pin name="RESETB" direction="pas"/>
<pin name="HOLDB" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="HOLDA" direction="pas"/>
<pin name="RESETA" direction="pas"/>
<pin name="SELECTA" direction="pas"/>
<pin name="SWCOMA" direction="pas"/>
<pin name="SWOUTA" direction="pas"/>
<pin name="OUTA" direction="out"/>
<pin name="GNDA" direction="pas"/>
<pin name="COMA" direction="in"/>
<pin name="CAPA" direction="pas"/>
<pin name="INA" direction="in"/>
<pin name="SWINA" direction="in"/>
</symbol>
<symbol name="ADC700">
<pin name="CMP-IN" direction="in"/>
<pin name="BPO" direction="pas"/>
<pin name="+VCC" direction="pas"/>
<pin name="G-ADJ" direction="pas"/>
<pin name="-VCC" direction="pas"/>
<pin name="/RESET" direction="in" function="dot"/>
<pin name="/WR" direction="in" function="dot"/>
<pin name="/RD" direction="in" function="dot"/>
<pin name="/CS" direction="in" function="dot"/>
<pin name="/HBEN" direction="in" function="dot"/>
<pin name="SDATA" direction="out"/>
<pin name="DRDY" direction="out"/>
<pin name="STATUS" direction="out"/>
<pin name="STRB" direction="out"/>
<pin name="DB8/0" direction="out"/>
<pin name="DB9/1" direction="out"/>
<pin name="DB10/2" direction="out"/>
<pin name="DB11/3" direction="out"/>
<pin name="DB12/4" direction="out"/>
<pin name="DB13/5" direction="out"/>
<pin name="DB14/6" direction="out"/>
<pin name="DB15/7" direction="out"/>
<pin name="/BTCEN" direction="in" function="dot"/>
<pin name="VDD" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="10V-RNG" direction="in"/>
<pin name="20V-RNG" direction="in"/>
</symbol>
<symbol name="ADC701">
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="+5V(D)@1" direction="pas"/>
<pin name="DGND@1" direction="pas"/>
<pin name="STROBE" direction="out"/>
<pin name="B-SEL" direction="in"/>
<pin name="CONVERT" direction="in"/>
<pin name="S&amp;H-CONT" direction="out"/>
<pin name="DGND@2" direction="pas"/>
<pin name="DGND@3" direction="pas"/>
<pin name="CLK-ADJ"/>
<pin name="DGND@4" direction="pas"/>
<pin name="+5V(D)@2" direction="pas"/>
<pin name="OFF-ADJ@"/>
<pin name="+15V" direction="pas"/>
<pin name="POWGND" direction="pas"/>
<pin name="-15V" direction="pas"/>
<pin name="IN-A" direction="in"/>
<pin name="IN-B" direction="in"/>
<pin name="SIGGND" direction="pas"/>
<pin name="IN-C" direction="in"/>
<pin name="IN-D" direction="in"/>
<pin name="REF-IN" direction="in"/>
<pin name="AGND@1" direction="pas"/>
<pin name="REFGND" direction="in"/>
<pin name="REF-OUT" direction="out"/>
<pin name="REF-ADJ" direction="in"/>
<pin name="+5V(A)" direction="pas"/>
<pin name="AGND@2" direction="pas"/>
<pin name="-5V(D)" direction="pas"/>
</symbol>
<symbol name="ADC7802">
<pin name="SFR" direction="pas"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="DGND" direction="pas"/>
<pin name="VA" direction="pas"/>
<pin name="D7" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D3/D11" direction="hiz"/>
<pin name="D2/D10" direction="hiz"/>
<pin name="D1/D9" direction="hiz"/>
<pin name="D0/D8" direction="hiz"/>
<pin name="/RD" direction="in"/>
<pin name="/CS" direction="in"/>
<pin name="/WR" direction="in"/>
<pin name="HBE" direction="in"/>
<pin name="/BUSY" direction="out"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="/CAL" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="VD" direction="pas"/>
</symbol>
<symbol name="ADS_574">
<pin name="+VDD" direction="pas"/>
<pin name="12/!8" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="NC" direction="pas"/>
<pin name="REF_OUT" direction="out"/>
<pin name="AGND" direction="pas"/>
<pin name="REF_IN" direction="in"/>
<pin name="VEE" direction="pas"/>
<pin name="B_OFFSET" direction="pas"/>
<pin name="10V" direction="pas"/>
<pin name="20V" direction="pas"/>
<pin name="DGND" direction="pas"/>
<pin name="D0" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="STATUS" direction="out"/>
</symbol>
<symbol name="ADS7805">
<pin name="+VDIG" direction="pas"/>
<pin name="+VANA" direction="pas"/>
<pin name="AGND2" direction="pas"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="D12" direction="out"/>
<pin name="D13" direction="out"/>
<pin name="D14" direction="out"/>
<pin name="D15" direction="out"/>
<pin name="VIN" direction="in"/>
<pin name="/BUSY" direction="out"/>
<pin name="/CS" direction="in"/>
<pin name="R/C" direction="pas"/>
<pin name="AGND1" direction="pas"/>
<pin name="REF" direction="pas"/>
<pin name="CAP" direction="pas"/>
<pin name="D3" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="DGND" direction="pas"/>
<pin name="BYTE" direction="in"/>
</symbol>
<symbol name="ADS7807">
<pin name="R1IN" direction="in"/>
<pin name="AGND1" direction="pas"/>
<pin name="R2IN" direction="in"/>
<pin name="CAP" direction="pas"/>
<pin name="REF" direction="pas"/>
<pin name="AGND2" direction="pas"/>
<pin name="SB/BTC" direction="in"/>
<pin name="EXT/INT" direction="in"/>
<pin name="D7" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="DGND" direction="pas"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="SCLK" direction="out"/>
<pin name="SDATA"/>
<pin name="TAG" direction="in"/>
<pin name="BYTE" direction="in"/>
<pin name="R/C" direction="out"/>
<pin name="CS" direction="in"/>
<pin name="BUSY" direction="in"/>
<pin name="PWRD" direction="in"/>
<pin name="REFD" direction="in"/>
<pin name="VANA" direction="in"/>
<pin name="VDIG" direction="in"/>
</symbol>
<symbol name="ADS7810">
<pin name="+VANA@1" direction="pas"/>
<pin name="+VANA@2" direction="pas"/>
<pin name="+VDIG@1" direction="pas"/>
<pin name="+VDIG@2" direction="pas"/>
<pin name="AGND2" direction="pas"/>
<pin name="DGND@1" direction="pas"/>
<pin name="DGND@2" direction="pas"/>
<pin name="-VANA" direction="pas"/>
<pin name="DO" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D7" direction="out"/>
<pin name="D8" direction="out"/>
<pin name="D9" direction="out"/>
<pin name="D10" direction="out"/>
<pin name="D11" direction="out"/>
<pin name="VIN" direction="in"/>
<pin name="BUSY" direction="out"/>
<pin name="R/C" direction="in"/>
<pin name="CS" direction="pas"/>
<pin name="AGND1" direction="pas"/>
<pin name="REF" direction="pas"/>
<pin name="CAP" direction="pas"/>
</symbol>
<symbol name="DAC707">
<pin name="VOUT" direction="in"/>
<pin name="VDD" direction="pas"/>
<pin name="DCOM" direction="in"/>
<pin name="ACOM" direction="in"/>
<pin name="SJ" direction="in"/>
<pin name="GA" direction="in"/>
<pin name="+VCC" direction="in"/>
<pin name="-VCC" direction="in"/>
<pin name="CLR" direction="in"/>
<pin name="WR" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="D15" direction="in"/>
<pin name="D14" direction="pas"/>
<pin name="D13" direction="out"/>
<pin name="D12" direction="pas"/>
<pin name="D11" direction="pas"/>
<pin name="D10" direction="pas"/>
<pin name="D9" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="pas"/>
<pin name="D6" direction="pas"/>
<pin name="D5" direction="pas"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="out"/>
<pin name="D2" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D0" direction="pas"/>
</symbol>
<symbol name="DAC729">
<pin name="MSB" direction="in"/>
<pin name="BIT2" direction="in"/>
<pin name="BIT3" direction="in"/>
<pin name="BIT4" direction="in"/>
<pin name="BIT5" direction="in"/>
<pin name="BIT6" direction="in"/>
<pin name="BIT7" direction="in"/>
<pin name="BIT8" direction="in"/>
<pin name="BIT9" direction="in"/>
<pin name="BIT10" direction="in"/>
<pin name="BIT11" direction="in"/>
<pin name="BIT12" direction="in"/>
<pin name="BIT13" direction="in"/>
<pin name="BIT14" direction="in"/>
<pin name="BIT15" direction="in"/>
<pin name="BIT16" direction="in"/>
<pin name="BIT17" direction="in"/>
<pin name="BIT18" direction="in"/>
<pin name="VDD" direction="pas"/>
<pin name="DGND" direction="in"/>
<pin name="VPOT" direction="out"/>
<pin name="B1_ADJ" direction="pas"/>
<pin name="B2_ADJ" direction="pas"/>
<pin name="B3_ADJ" direction="pas"/>
<pin name="B4_ADJ" direction="pas"/>
<pin name="REF_ADJ" direction="pas"/>
<pin name="REF_OUT" direction="out"/>
<pin name="REF_IN" direction="in"/>
<pin name="AGND" direction="pas"/>
<pin name="-VCC" direction="pas"/>
<pin name="+VCC" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="SJ" direction="pas"/>
<pin name="GAIN_ADJ" direction="pas"/>
<pin name="REF_GND" direction="pas"/>
<pin name="10K@1" direction="pas"/>
<pin name="10K@2" direction="pas"/>
<pin name="5K@1" direction="pas"/>
<pin name="5K@2" direction="pas"/>
<pin name="IOUT" direction="out"/>
</symbol>
<symbol name="DAC80P-I">
<pin name="MSB" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="LSB" direction="in"/>
<pin name="-VCC" direction="pas"/>
<pin name="IOUT" direction="pas"/>
<pin name="REFIN" direction="in"/>
<pin name="BIPOL" direction="pas"/>
<pin name="NET@1" direction="pas"/>
<pin name="NET@2" direction="pas"/>
<pin name="NET@3" direction="pas"/>
<pin name="COMMON" direction="pas"/>
<pin name="+VCC" direction="pas"/>
<pin name="GAIN" direction="pas"/>
<pin name="REFOUT" direction="out"/>
</symbol>
<symbol name="DF1700">
<pin name="SDI" direction="in"/>
<pin name="BCKI" direction="in"/>
<pin name="CKSL" direction="pas"/>
<pin name="CKDV" direction="pas"/>
<pin name="XTI" direction="in"/>
<pin name="VSS" direction="pas"/>
<pin name="SYN" direction="pas"/>
<pin name="RST" direction="pas"/>
<pin name="/OW20"/>
<pin name="/OW18"/>
<pin name="VSS@2" direction="pas"/>
<pin name="VDD" direction="pas"/>
<pin name="DOR" direction="out"/>
<pin name="DOL" direction="out"/>
<pin name="WCKO" direction="out"/>
<pin name="BCKO" direction="out"/>
<pin name="LRCI" direction="in"/>
</symbol>
<symbol name="HPR_105">
<pin name="VIN" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="V+" direction="pas"/>
</symbol>
<symbol name="HPR117">
<pin name="+VIN" direction="pas"/>
<pin name="-VIN" direction="pas"/>
<pin name="-VOUT" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="+VOUT" direction="pas"/>
</symbol>
<symbol name="HPR1XX">
<pin name="-VIN" direction="pas"/>
<pin name="+VIN" direction="pas"/>
<pin name="-VOUT" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="+VOUT" direction="pas"/>
</symbol>
<symbol name="INA101_G">
<pin name="OUT" direction="out"/>
<pin name="+VCC" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="SENSE1" direction="in"/>
<pin name="GSET1" direction="pas"/>
<pin name="OADJ@1" direction="pas"/>
<pin name="OADJ@2" direction="pas"/>
<pin name="GSET2" direction="pas"/>
<pin name="SENSE2" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="-VCC" direction="out"/>
<pin name="COMMON" direction="pas"/>
</symbol>
<symbol name="INA102">
<pin name="OFFADJ@1" direction="pas"/>
<pin name="*10" direction="pas"/>
<pin name="*100" direction="pas"/>
<pin name="*1000" direction="pas"/>
<pin name="*1000GS" direction="pas"/>
<pin name="G_SENSE" direction="pas"/>
<pin name="G_SET" direction="pas"/>
<pin name="CMRTRIM" direction="pas"/>
<pin name="-VCC" direction="pas"/>
<pin name="COMMON" direction="in"/>
<pin name="OUTPUT" direction="out"/>
<pin name="+VCC" direction="pas"/>
<pin name="FILTER" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OFFADJ@2" direction="pas"/>
</symbol>
<symbol name="INA105P">
<pin name="REF" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="SENSE" direction="pas"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="INA110">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="O_IN@1" direction="pas"/>
<pin name="O_IN@2" direction="pas"/>
<pin name="REF" direction="in"/>
<pin name="OUTPUT" direction="out"/>
<pin name="SENSE" direction="in"/>
<pin name="*500" direction="pas"/>
<pin name="*100" direction="pas"/>
<pin name="*10" direction="pas"/>
<pin name="O_OUT@1" direction="pas"/>
<pin name="O_OUT@2" direction="pas"/>
<pin name="*200" direction="pas"/>
</symbol>
<symbol name="INA110KP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="OFFIN@1" direction="pas"/>
<pin name="OFFIN@2" direction="pas"/>
<pin name="REF" direction="pas"/>
<pin name="-VCC" direction="pas"/>
<pin name="+VCC" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="SENSE" direction="pas"/>
<pin name="*500" direction="pas"/>
<pin name="*100" direction="pas"/>
<pin name="*10" direction="pas"/>
<pin name="OFFOUT@1" direction="pas"/>
<pin name="OFFOUT@2" direction="pas"/>
<pin name="*200" direction="pas"/>
</symbol>
<symbol name="ISO485P">
<pin name="R" direction="in"/>
<pin name="D" direction="out"/>
<pin name="A"/>
<pin name="B"/>
<pin name="RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="PWR2">
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="XTR101A">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="SPAN_0" direction="pas"/>
<pin name="SPAN_1" direction="pas"/>
<pin name="IREF1" direction="in"/>
<pin name="IREF2" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="BW" direction="out"/>
<pin name="E" direction="out"/>
<pin name="ZADJ" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="ZA_0" direction="pas"/>
<pin name="ZA_1" direction="pas"/>
<pin name="B" direction="out"/>
</symbol>
<symbol name="INA138">
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="ADS8344">
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="!SHDN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="DOUT" direction="out"/>
<pin name="DI" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="BUSY" direction="out"/>
</symbol>
<symbol name="+-VCC">
<pin name="+VCC" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
</symbol>
<symbol name="PCM1792">
<pin name="MSEL" direction="in"/>
<pin name="LRCK" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="MDI" direction="in"/>
<pin name="!MS" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="BCK" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="IOUTL-" direction="out"/>
<pin name="IOUTL+" direction="out"/>
<pin name="IREF" direction="pas"/>
<pin name="ZEROL" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="AGND3L" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCOML" direction="pas"/>
<pin name="ZEROR" direction="out"/>
<pin name="MDO" direction="out"/>
<pin name="!RST" direction="in"/>
<pin name="VCC2L" direction="pwr"/>
<pin name="VCOMR" direction="pas"/>
<pin name="IOUTR+" direction="out"/>
<pin name="IOUTR-" direction="out"/>
<pin name="AGND1" direction="pwr"/>
<pin name="AGND3R" direction="pwr"/>
<pin name="VCC2R" direction="pwr"/>
</symbol>
<symbol name="PCM1793">
<pin name="DEMP0" direction="in"/>
<pin name="LRCK" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="FMT0" direction="in"/>
<pin name="FMT2" direction="in"/>
<pin name="FMT1" direction="in"/>
<pin name="BCK" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="VOUTL-" direction="out"/>
<pin name="VOUTL+" direction="out"/>
<pin name="ZEROL" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VCCF" direction="pwr"/>
<pin name="AGNDC" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VCCC" direction="pwr"/>
<pin name="VCOM" direction="pas"/>
<pin name="ZEROR" direction="out"/>
<pin name="DEMP1" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="VCCL" direction="pwr"/>
<pin name="VOUTR+" direction="out"/>
<pin name="VOUTR-" direction="out"/>
<pin name="AGNDL" direction="pwr"/>
<pin name="AGNDR" direction="pwr"/>
<pin name="VCCR" direction="pwr"/>
<pin name="AGNDF" direction="pwr"/>
<pin name="MUTE" direction="in"/>
</symbol>
<symbol name="BUF602">
<pin name="VREF" direction="pas"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="RCV420">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="RCVCOM" direction="in"/>
<pin name="REFCOM" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="V-" direction="in"/>
<pin name="REFIN" direction="in"/>
<pin name="RCVFB" direction="in"/>
<pin name="RCVOUT" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="REFFB" direction="in"/>
<pin name="REFTRIMM" direction="in"/>
<pin name="REFNOISE" direction="in"/>
</symbol>
<symbol name="ADS7828">
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="SDA"/>
<pin name="REFIN/REFOUT" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="SCL" direction="in"/>
</symbol>
<symbol name="INA163">
<pin name="-IN" direction="in"/>
<pin name="GS1" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GS2" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="REF" direction="pas"/>
<pin name="VO1" direction="pas"/>
<pin name="VO2" direction="pas"/>
<pin name="SENSE" direction="pas"/>
</symbol>
<symbol name="INA217">
<pin name="-IN" direction="in"/>
<pin name="RG1" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RG2" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="REF" direction="pas"/>
</symbol>
<symbol name="PGA2500">
<pin name="GPO1" direction="out"/>
<pin name="GPO2" direction="out"/>
<pin name="GPO3" direction="out"/>
<pin name="GPO4" direction="out"/>
<pin name="OVR" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="!DCEN" direction="in"/>
<pin name="0DB" direction="in"/>
<pin name="ZCEN" direction="in"/>
<pin name="SDI" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="SDO" direction="out"/>
<pin name="VD-" direction="pwr"/>
<pin name="VA-" direction="pwr"/>
<pin name="VOUT-" direction="out"/>
<pin name="VOUT+" direction="out"/>
<pin name="VA+" direction="pwr"/>
<pin name="VA+@1" direction="pwr"/>
<pin name="VA-@1" direction="pwr"/>
<pin name="CS22" direction="pas"/>
<pin name="CS21" direction="pas"/>
<pin name="CS12" direction="pas"/>
<pin name="CS11" direction="pas"/>
<pin name="VCOMIN" direction="pwr"/>
<pin name="VIN-" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="AGND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="INA2128" prefix="IC">
<description>&lt;b&gt;Dual Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Low Power</description>
<gates>
<gate name="G$1" symbol="INA2128"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="INA+" pad="2"/>
<connect gate="G$1" pin="INA-" pad="1"/>
<connect gate="G$1" pin="INB+" pad="15"/>
<connect gate="G$1" pin="INB-" pad="16"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="12"/>
<connect gate="G$1" pin="RGA" pad="3"/>
<connect gate="G$1" pin="RGA@1" pad="4"/>
<connect gate="G$1" pin="RGB" pad="13"/>
<connect gate="G$1" pin="RGB@1" pad="14"/>
<connect gate="G$1" pin="SENSEA" pad="7"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VOA" pad="6"/>
<connect gate="G$1" pin="VOB" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="INA+" pad="2"/>
<connect gate="G$1" pin="INA-" pad="1"/>
<connect gate="G$1" pin="INB+" pad="15"/>
<connect gate="G$1" pin="INB-" pad="16"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="12"/>
<connect gate="G$1" pin="RGA" pad="3"/>
<connect gate="G$1" pin="RGA@1" pad="4"/>
<connect gate="G$1" pin="RGB" pad="13"/>
<connect gate="G$1" pin="RGB@1" pad="14"/>
<connect gate="G$1" pin="SENSEA" pad="7"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VOA" pad="6"/>
<connect gate="G$1" pin="VOB" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA2128U"/>
<attribute name="OC_FARNELL" value="1212421"/>
<attribute name="OC_NEWARK" value="28C7388"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA2141" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Dual, Low Power, G = 10, 100</description>
<gates>
<gate name="G$1" symbol="INA2141"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="INA+" pad="2"/>
<connect gate="G$1" pin="INA-" pad="1"/>
<connect gate="G$1" pin="INB+" pad="15"/>
<connect gate="G$1" pin="INB-" pad="16"/>
<connect gate="G$1" pin="JA" pad="3"/>
<connect gate="G$1" pin="JA@1" pad="4"/>
<connect gate="G$1" pin="JB" pad="13"/>
<connect gate="G$1" pin="JB@1" pad="14"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="12"/>
<connect gate="G$1" pin="SENSEA" pad="7"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VOA" pad="6"/>
<connect gate="G$1" pin="VOB" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="INA+" pad="2"/>
<connect gate="G$1" pin="INA-" pad="1"/>
<connect gate="G$1" pin="INB+" pad="15"/>
<connect gate="G$1" pin="INB-" pad="16"/>
<connect gate="G$1" pin="JA" pad="3"/>
<connect gate="G$1" pin="JA@1" pad="4"/>
<connect gate="G$1" pin="JB" pad="13"/>
<connect gate="G$1" pin="JB@1" pad="14"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="12"/>
<connect gate="G$1" pin="SENSEA" pad="7"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VOA" pad="6"/>
<connect gate="G$1" pin="VOB" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA2141U"/>
<attribute name="OC_FARNELL" value="1459468"/>
<attribute name="OC_NEWARK" value="74C9853"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO130?B" prefix="IC">
<description>&lt;b&gt;Isolation Amplifier&lt;/b&gt;&lt;p&gt;
Precision, Lowest Cost</description>
<gates>
<gate name="G$1" symbol="ISO130"/>
</gates>
<devices>
<device name="U" package="SO08-GW">
<connects>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="IN+" pad="2"/>
<connect gate="G$1" pin="IN-" pad="3"/>
<connect gate="G$1" pin="OUT+" pad="7"/>
<connect gate="G$1" pin="OUT-" pad="6"/>
<connect gate="G$1" pin="VS1" pad="1"/>
<connect gate="G$1" pin="VS2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="IN+" pad="2"/>
<connect gate="G$1" pin="IN-" pad="3"/>
<connect gate="G$1" pin="OUT+" pad="7"/>
<connect gate="G$1" pin="OUT-" pad="6"/>
<connect gate="G$1" pin="VS1" pad="1"/>
<connect gate="G$1" pin="VS2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7821" prefix="IC">
<description>&lt;b&gt;16-Bit 10us Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7821"/>
</gates>
<devices>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="26"/>
<connect gate="G$1" pin="!CS" pad="25"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="23"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="22"/>
<connect gate="G$1" pin="D1" pad="21"/>
<connect gate="G$1" pin="D10" pad="11"/>
<connect gate="G$1" pin="D11" pad="10"/>
<connect gate="G$1" pin="D12" pad="9"/>
<connect gate="G$1" pin="D13" pad="8"/>
<connect gate="G$1" pin="D14" pad="7"/>
<connect gate="G$1" pin="D15" pad="6"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="19"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="16"/>
<connect gate="G$1" pin="D7" pad="15"/>
<connect gate="G$1" pin="D8" pad="13"/>
<connect gate="G$1" pin="D9" pad="12"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="R/!C" pad="24"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="26"/>
<connect gate="G$1" pin="!CS" pad="25"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="23"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="22"/>
<connect gate="G$1" pin="D1" pad="21"/>
<connect gate="G$1" pin="D10" pad="11"/>
<connect gate="G$1" pin="D11" pad="10"/>
<connect gate="G$1" pin="D12" pad="9"/>
<connect gate="G$1" pin="D13" pad="8"/>
<connect gate="G$1" pin="D14" pad="7"/>
<connect gate="G$1" pin="D15" pad="6"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="19"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="16"/>
<connect gate="G$1" pin="D7" pad="15"/>
<connect gate="G$1" pin="D8" pad="13"/>
<connect gate="G$1" pin="D9" pad="12"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="R/!C" pad="24"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7820" prefix="IC">
<description>&lt;b&gt;12-Bit 10us Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7820"/>
</gates>
<devices>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="26"/>
<connect gate="G$1" pin="!CS" pad="25"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="23"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="7"/>
<connect gate="G$1" pin="D11" pad="6"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="D8" pad="9"/>
<connect gate="G$1" pin="D9" pad="8"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DZ" pad="19"/>
<connect gate="G$1" pin="DZ@1" pad="20"/>
<connect gate="G$1" pin="DZ@2" pad="21"/>
<connect gate="G$1" pin="DZ@3" pad="22"/>
<connect gate="G$1" pin="R/!C" pad="24"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="26"/>
<connect gate="G$1" pin="!CS" pad="25"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="23"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="7"/>
<connect gate="G$1" pin="D11" pad="6"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="D8" pad="9"/>
<connect gate="G$1" pin="D9" pad="8"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DZ" pad="19"/>
<connect gate="G$1" pin="DZ@1" pad="20"/>
<connect gate="G$1" pin="DZ@2" pad="21"/>
<connect gate="G$1" pin="DZ@3" pad="22"/>
<connect gate="G$1" pin="R/!C" pad="24"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7812" prefix="IC">
<description>&lt;b&gt;Low-Power, Serial 12-Bit Sampling ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7812"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!BUSY" pad="14"/>
<connect gate="G$1" pin="!CONV" pad="12"/>
<connect gate="G$1" pin="!CS" pad="13"/>
<connect gate="G$1" pin="BUF" pad="5"/>
<connect gate="G$1" pin="CAP" pad="6"/>
<connect gate="G$1" pin="DATA" pad="10"/>
<connect gate="G$1" pin="DATACLK" pad="9"/>
<connect gate="G$1" pin="EXT/!INT" pad="11"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PWRD" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="R3IN" pad="4"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="VS" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS7812P"/>
<attribute name="OC_FARNELL" value="1509513"/>
<attribute name="OC_NEWARK" value="74C7091"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="!BUSY" pad="14"/>
<connect gate="G$1" pin="!CONV" pad="12"/>
<connect gate="G$1" pin="!CS" pad="13"/>
<connect gate="G$1" pin="BUF" pad="5"/>
<connect gate="G$1" pin="CAP" pad="6"/>
<connect gate="G$1" pin="DATA" pad="10"/>
<connect gate="G$1" pin="DATACLK" pad="9"/>
<connect gate="G$1" pin="EXT/!INT" pad="11"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PWRD" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="R3IN" pad="4"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="VS" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS7812U"/>
<attribute name="OC_FARNELL" value="1459274"/>
<attribute name="OC_NEWARK" value="14M8148"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7805" prefix="IC">
<description>&lt;b&gt;16-Bit 10us Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7821"/>
</gates>
<devices>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="26"/>
<connect gate="G$1" pin="!CS" pad="25"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="23"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="22"/>
<connect gate="G$1" pin="D1" pad="21"/>
<connect gate="G$1" pin="D10" pad="11"/>
<connect gate="G$1" pin="D11" pad="10"/>
<connect gate="G$1" pin="D12" pad="9"/>
<connect gate="G$1" pin="D13" pad="8"/>
<connect gate="G$1" pin="D14" pad="7"/>
<connect gate="G$1" pin="D15" pad="6"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="19"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="16"/>
<connect gate="G$1" pin="D7" pad="15"/>
<connect gate="G$1" pin="D8" pad="13"/>
<connect gate="G$1" pin="D9" pad="12"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="R/!C" pad="24"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7805P"/>
<attribute name="OC_FARNELL" value="1212283"/>
<attribute name="OC_NEWARK" value="35C1528"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="26"/>
<connect gate="G$1" pin="!CS" pad="25"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="23"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="22"/>
<connect gate="G$1" pin="D1" pad="21"/>
<connect gate="G$1" pin="D10" pad="11"/>
<connect gate="G$1" pin="D11" pad="10"/>
<connect gate="G$1" pin="D12" pad="9"/>
<connect gate="G$1" pin="D13" pad="8"/>
<connect gate="G$1" pin="D14" pad="7"/>
<connect gate="G$1" pin="D15" pad="6"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="19"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="16"/>
<connect gate="G$1" pin="D7" pad="15"/>
<connect gate="G$1" pin="D8" pad="13"/>
<connect gate="G$1" pin="D9" pad="12"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="R/!C" pad="24"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7805U"/>
<attribute name="OC_FARNELL" value="1192284"/>
<attribute name="OC_NEWARK" value="80K5546"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IVC102U" prefix="IC">
<description>&lt;b&gt;Amplifier&lt;/b&gt;&lt;p&gt;
Precision Switched Integrator Transimpedance</description>
<gates>
<gate name="G$1" symbol="IVC102"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="C1" pad="4"/>
<connect gate="G$1" pin="C2" pad="5"/>
<connect gate="G$1" pin="C3" pad="6"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC@1" pad="8"/>
<connect gate="G$1" pin="S1" pad="11"/>
<connect gate="G$1" pin="S2" pad="12"/>
<connect gate="G$1" pin="V+" pad="14"/>
<connect gate="G$1" pin="V-" pad="9"/>
<connect gate="G$1" pin="VOUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="IVC102U"/>
<attribute name="OC_FARNELL" value="1212427"/>
<attribute name="OC_NEWARK" value="03P0868"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO122" prefix="IC">
<description>&lt;b&gt;Isolation Amplifier&lt;/b&gt;&lt;p&gt;
Precision, Lowest Cost</description>
<gates>
<gate name="G$1" symbol="ISO122"/>
</gates>
<devices>
<device name="P" package="DIL16/8">
<connects>
<connect gate="G$1" pin="+VS1" pad="1"/>
<connect gate="G$1" pin="+VS2" pad="9"/>
<connect gate="G$1" pin="-VS1" pad="2"/>
<connect gate="G$1" pin="-VS2" pad="10"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO122P"/>
<attribute name="OC_FARNELL" value="1520510"/>
<attribute name="OC_NEWARK" value="55M8194"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3/8">
<connects>
<connect gate="G$1" pin="+VS1" pad="1"/>
<connect gate="G$1" pin="+VS2" pad="15"/>
<connect gate="G$1" pin="-VS1" pad="2"/>
<connect gate="G$1" pin="-VS2" pad="16"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="VIN" pad="27"/>
<connect gate="G$1" pin="VOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO122UE4"/>
<attribute name="OC_FARNELL" value="1206915"/>
<attribute name="OC_NEWARK" value="61K0056"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO124" prefix="IC">
<description>&lt;b&gt;Isolation Amplifier&lt;/b&gt;&lt;p&gt;
Precision, Lowest Cost</description>
<gates>
<gate name="G$1" symbol="ISO122"/>
</gates>
<devices>
<device name="P" package="DIL16/8">
<connects>
<connect gate="G$1" pin="+VS1" pad="1"/>
<connect gate="G$1" pin="+VS2" pad="9"/>
<connect gate="G$1" pin="-VS1" pad="2"/>
<connect gate="G$1" pin="-VS2" pad="10"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VOUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ISO124P"/>
<attribute name="OC_FARNELL" value="1212425"/>
<attribute name="OC_NEWARK" value="35C1752"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3/8">
<connects>
<connect gate="G$1" pin="+VS1" pad="1"/>
<connect gate="G$1" pin="+VS2" pad="15"/>
<connect gate="G$1" pin="-VS1" pad="2"/>
<connect gate="G$1" pin="-VS2" pad="16"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="VIN" pad="27"/>
<connect gate="G$1" pin="VOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ISO124U"/>
<attribute name="OC_FARNELL" value="1212426"/>
<attribute name="OC_NEWARK" value="10M8426"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPC506A" prefix="IC">
<description>&lt;b&gt;CMOS Analog Multiplexers&lt;/b&gt;&lt;p&gt;
Single-Ended 16-Channel/Differential 8-Channel</description>
<gates>
<gate name="G$1" symbol="MPC506"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="+V" pad="1"/>
<connect gate="G$1" pin="-V" pad="27"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="ENABLE" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="IN1" pad="19"/>
<connect gate="G$1" pin="IN10" pad="10"/>
<connect gate="G$1" pin="IN11" pad="9"/>
<connect gate="G$1" pin="IN12" pad="8"/>
<connect gate="G$1" pin="IN13" pad="7"/>
<connect gate="G$1" pin="IN14" pad="6"/>
<connect gate="G$1" pin="IN15" pad="5"/>
<connect gate="G$1" pin="IN16" pad="4"/>
<connect gate="G$1" pin="IN2" pad="20"/>
<connect gate="G$1" pin="IN3" pad="21"/>
<connect gate="G$1" pin="IN4" pad="22"/>
<connect gate="G$1" pin="IN5" pad="23"/>
<connect gate="G$1" pin="IN6" pad="24"/>
<connect gate="G$1" pin="IN7" pad="25"/>
<connect gate="G$1" pin="IN8" pad="26"/>
<connect gate="G$1" pin="IN9" pad="11"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="OUT" pad="28"/>
<connect gate="G$1" pin="VREF" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MPC506AP"/>
<attribute name="OC_FARNELL" value="1417416"/>
<attribute name="OC_NEWARK" value="50R5624"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="+V" pad="1"/>
<connect gate="G$1" pin="-V" pad="27"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="14"/>
<connect gate="G$1" pin="ENABLE" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="IN1" pad="19"/>
<connect gate="G$1" pin="IN10" pad="10"/>
<connect gate="G$1" pin="IN11" pad="9"/>
<connect gate="G$1" pin="IN12" pad="8"/>
<connect gate="G$1" pin="IN13" pad="7"/>
<connect gate="G$1" pin="IN14" pad="6"/>
<connect gate="G$1" pin="IN15" pad="5"/>
<connect gate="G$1" pin="IN16" pad="4"/>
<connect gate="G$1" pin="IN2" pad="20"/>
<connect gate="G$1" pin="IN3" pad="21"/>
<connect gate="G$1" pin="IN4" pad="22"/>
<connect gate="G$1" pin="IN5" pad="23"/>
<connect gate="G$1" pin="IN6" pad="24"/>
<connect gate="G$1" pin="IN7" pad="25"/>
<connect gate="G$1" pin="IN8" pad="26"/>
<connect gate="G$1" pin="IN9" pad="11"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="OUT" pad="28"/>
<connect gate="G$1" pin="VREF" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="MPC506AU"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="72K8921"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPC507A" prefix="IC">
<description>&lt;b&gt;CMOS Analog Multiplexers&lt;/b&gt;&lt;p&gt;
Single-Ended 16-Channel/Differential 8-Channel</description>
<gates>
<gate name="G$1" symbol="MPC507"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="+V" pad="1"/>
<connect gate="G$1" pin="-V" pad="27"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="ENABLE" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="IN1A" pad="19"/>
<connect gate="G$1" pin="IN1B" pad="11"/>
<connect gate="G$1" pin="IN2A" pad="20"/>
<connect gate="G$1" pin="IN2B" pad="10"/>
<connect gate="G$1" pin="IN3A" pad="21"/>
<connect gate="G$1" pin="IN3B" pad="9"/>
<connect gate="G$1" pin="IN4A" pad="22"/>
<connect gate="G$1" pin="IN4B" pad="8"/>
<connect gate="G$1" pin="IN5A" pad="23"/>
<connect gate="G$1" pin="IN5B" pad="7"/>
<connect gate="G$1" pin="IN6A" pad="24"/>
<connect gate="G$1" pin="IN6B" pad="6"/>
<connect gate="G$1" pin="IN7A" pad="25"/>
<connect gate="G$1" pin="IN7B" pad="5"/>
<connect gate="G$1" pin="IN8A" pad="26"/>
<connect gate="G$1" pin="IN8B" pad="4"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="14"/>
<connect gate="G$1" pin="OUTA" pad="28"/>
<connect gate="G$1" pin="OUTB" pad="2"/>
<connect gate="G$1" pin="VREF" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="MPC507AP"/>
<attribute name="OC_FARNELL" value="1648762"/>
<attribute name="OC_NEWARK" value="75C3662"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="+V" pad="1"/>
<connect gate="G$1" pin="-V" pad="27"/>
<connect gate="G$1" pin="A0" pad="17"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="ENABLE" pad="18"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="IN1A" pad="19"/>
<connect gate="G$1" pin="IN1B" pad="11"/>
<connect gate="G$1" pin="IN2A" pad="20"/>
<connect gate="G$1" pin="IN2B" pad="10"/>
<connect gate="G$1" pin="IN3A" pad="21"/>
<connect gate="G$1" pin="IN3B" pad="9"/>
<connect gate="G$1" pin="IN4A" pad="22"/>
<connect gate="G$1" pin="IN4B" pad="8"/>
<connect gate="G$1" pin="IN5A" pad="23"/>
<connect gate="G$1" pin="IN5B" pad="7"/>
<connect gate="G$1" pin="IN6A" pad="24"/>
<connect gate="G$1" pin="IN6B" pad="6"/>
<connect gate="G$1" pin="IN7A" pad="25"/>
<connect gate="G$1" pin="IN7B" pad="5"/>
<connect gate="G$1" pin="IN8A" pad="26"/>
<connect gate="G$1" pin="IN8B" pad="4"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="14"/>
<connect gate="G$1" pin="OUTA" pad="28"/>
<connect gate="G$1" pin="OUTB" pad="2"/>
<connect gate="G$1" pin="VREF" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="MPC507AU"/>
<attribute name="OC_FARNELL" value="1577157"/>
<attribute name="OC_NEWARK" value="75C3663"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPC508A" prefix="IC">
<description>&lt;b&gt;CMOS Analog Multiplexers&lt;/b&gt;&lt;p&gt;
Single-Ended 8-Channel/Differential 4-Channell</description>
<gates>
<gate name="G$1" symbol="MPC508"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+V" pad="13"/>
<connect gate="G$1" pin="-V" pad="3"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="6"/>
<connect gate="G$1" pin="IN4" pad="7"/>
<connect gate="G$1" pin="IN5" pad="12"/>
<connect gate="G$1" pin="IN6" pad="11"/>
<connect gate="G$1" pin="IN7" pad="10"/>
<connect gate="G$1" pin="IN8" pad="9"/>
<connect gate="G$1" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="MPC508AP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4520"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+V" pad="13"/>
<connect gate="G$1" pin="-V" pad="3"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="14"/>
<connect gate="G$1" pin="IN1" pad="4"/>
<connect gate="G$1" pin="IN2" pad="5"/>
<connect gate="G$1" pin="IN3" pad="6"/>
<connect gate="G$1" pin="IN4" pad="7"/>
<connect gate="G$1" pin="IN5" pad="12"/>
<connect gate="G$1" pin="IN6" pad="11"/>
<connect gate="G$1" pin="IN7" pad="10"/>
<connect gate="G$1" pin="IN8" pad="9"/>
<connect gate="G$1" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="MPC508AU"/>
<attribute name="OC_FARNELL" value="1206920"/>
<attribute name="OC_NEWARK" value="74K3896"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MPC509A" prefix="IC">
<description>&lt;b&gt;CMOS Analog Multiplexers&lt;/b&gt;&lt;p&gt;
Single-Ended 8-Channel/Differential 4-Channel</description>
<gates>
<gate name="G$1" symbol="MPC509"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+V" pad="14"/>
<connect gate="G$1" pin="-V" pad="3"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="IN1A" pad="4"/>
<connect gate="G$1" pin="IN1B" pad="13"/>
<connect gate="G$1" pin="IN2A" pad="5"/>
<connect gate="G$1" pin="IN2B" pad="12"/>
<connect gate="G$1" pin="IN3A" pad="6"/>
<connect gate="G$1" pin="IN3B" pad="11"/>
<connect gate="G$1" pin="IN4A" pad="7"/>
<connect gate="G$1" pin="IN4B" pad="10"/>
<connect gate="G$1" pin="OUTA" pad="8"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="MPC509AP"/>
<attribute name="OC_FARNELL" value="1214449"/>
<attribute name="OC_NEWARK" value="75C3667"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+V" pad="14"/>
<connect gate="G$1" pin="-V" pad="3"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="EN" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="IN1A" pad="4"/>
<connect gate="G$1" pin="IN1B" pad="13"/>
<connect gate="G$1" pin="IN2A" pad="5"/>
<connect gate="G$1" pin="IN2B" pad="12"/>
<connect gate="G$1" pin="IN3A" pad="6"/>
<connect gate="G$1" pin="IN3B" pad="11"/>
<connect gate="G$1" pin="IN4A" pad="7"/>
<connect gate="G$1" pin="IN4B" pad="10"/>
<connect gate="G$1" pin="OUTA" pad="8"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MPC509AUG4"/>
<attribute name="OC_FARNELL" value="1206921"/>
<attribute name="OC_NEWARK" value="97K5354"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO164" prefix="IC">
<description>&lt;b&gt;Isolated Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ISO164"/>
</gates>
<devices>
<device name="P" package="DIL24/16">
<connects>
<connect gate="G$1" pin="A0" pad="23"/>
<connect gate="G$1" pin="A1" pad="24"/>
<connect gate="G$1" pin="COM1/S1" pad="5"/>
<connect gate="G$1" pin="COM2" pad="10"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="20"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="IN+" pad="4"/>
<connect gate="G$1" pin="IN-" pad="3"/>
<connect gate="G$1" pin="OSC" pad="21"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="VS1+" pad="1"/>
<connect gate="G$1" pin="VS1-" pad="2"/>
<connect gate="G$1" pin="VS2+" pad="15"/>
<connect gate="G$1" pin="VS2-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO174" prefix="IC">
<description>&lt;b&gt;Isolated Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ISO164"/>
</gates>
<devices>
<device name="P" package="DIL24/16">
<connects>
<connect gate="G$1" pin="A0" pad="23"/>
<connect gate="G$1" pin="A1" pad="24"/>
<connect gate="G$1" pin="COM1/S1" pad="5"/>
<connect gate="G$1" pin="COM2" pad="10"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="GND1" pad="20"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="IN+" pad="4"/>
<connect gate="G$1" pin="IN-" pad="3"/>
<connect gate="G$1" pin="OSC" pad="21"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="VS1+" pad="1"/>
<connect gate="G$1" pin="VS1-" pad="2"/>
<connect gate="G$1" pin="VS2+" pad="15"/>
<connect gate="G$1" pin="VS2-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO165" prefix="IC">
<description>&lt;b&gt;Isolated Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ISO165"/>
</gates>
<devices>
<device name="R" package="D24-3/16">
<connects>
<connect gate="G$1" pin="COM1" pad="23"/>
<connect gate="G$1" pin="COM2" pad="10"/>
<connect gate="G$1" pin="FBN" pad="2"/>
<connect gate="G$1" pin="FBP" pad="22"/>
<connect gate="G$1" pin="GND1" pad="20"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="IN+" pad="24"/>
<connect gate="G$1" pin="IN-" pad="1"/>
<connect gate="G$1" pin="OSC" pad="21"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="S1" pad="5"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="VS1+" pad="4"/>
<connect gate="G$1" pin="VS1-" pad="3"/>
<connect gate="G$1" pin="VS2+" pad="15"/>
<connect gate="G$1" pin="VS2-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO175" prefix="IC">
<description>&lt;b&gt;Isolated Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Precision</description>
<gates>
<gate name="G$1" symbol="ISO165"/>
</gates>
<devices>
<device name="P" package="D24-3/16">
<connects>
<connect gate="G$1" pin="COM1" pad="23"/>
<connect gate="G$1" pin="COM2" pad="10"/>
<connect gate="G$1" pin="FBN" pad="2"/>
<connect gate="G$1" pin="FBP" pad="22"/>
<connect gate="G$1" pin="GND1" pad="20"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="IN+" pad="24"/>
<connect gate="G$1" pin="IN-" pad="1"/>
<connect gate="G$1" pin="OSC" pad="21"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="S1" pad="5"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="VS1+" pad="4"/>
<connect gate="G$1" pin="VS1-" pad="3"/>
<connect gate="G$1" pin="VS2+" pad="15"/>
<connect gate="G$1" pin="VS2-" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO166" prefix="IC">
<description>&lt;b&gt;Isolated Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ISO166"/>
</gates>
<devices>
<device name="P" package="D24-3/16">
<connects>
<connect gate="G$1" pin="+VS1" pad="4"/>
<connect gate="G$1" pin="+VS2" pad="15"/>
<connect gate="G$1" pin="-VS1" pad="3"/>
<connect gate="G$1" pin="-VS2" pad="13"/>
<connect gate="G$1" pin="COM1" pad="23"/>
<connect gate="G$1" pin="COM2" pad="10"/>
<connect gate="G$1" pin="GND1" pad="20"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="IN+" pad="1"/>
<connect gate="G$1" pin="IN-" pad="24"/>
<connect gate="G$1" pin="MOD" pad="21"/>
<connect gate="G$1" pin="OSC" pad="22"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="S1" pad="5"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO176" prefix="IC">
<description>&lt;b&gt;Isolated Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="ISO166"/>
</gates>
<devices>
<device name="P" package="D24-3/16">
<connects>
<connect gate="G$1" pin="+VS1" pad="4"/>
<connect gate="G$1" pin="+VS2" pad="15"/>
<connect gate="G$1" pin="-VS1" pad="3"/>
<connect gate="G$1" pin="-VS2" pad="13"/>
<connect gate="G$1" pin="COM1" pad="23"/>
<connect gate="G$1" pin="COM2" pad="10"/>
<connect gate="G$1" pin="GND1" pad="20"/>
<connect gate="G$1" pin="GND2" pad="12"/>
<connect gate="G$1" pin="IN+" pad="1"/>
<connect gate="G$1" pin="IN-" pad="24"/>
<connect gate="G$1" pin="MOD" pad="21"/>
<connect gate="G$1" pin="OSC" pad="22"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="S1" pad="5"/>
<connect gate="G$1" pin="S2" pad="14"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AFE1115" prefix="IC">
<description>&lt;b&gt;HDSL/MDSL Analog Front End with VCXO&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AFE1115"/>
</gates>
<devices>
<device name="E" package="SSOP56DL">
<connects>
<connect gate="G$1" pin="AGND" pad="36"/>
<connect gate="G$1" pin="AGND@1" pad="37"/>
<connect gate="G$1" pin="AGND@2" pad="42"/>
<connect gate="G$1" pin="AGND@3" pad="46"/>
<connect gate="G$1" pin="AGND@4" pad="48"/>
<connect gate="G$1" pin="AGND@5" pad="49"/>
<connect gate="G$1" pin="AVDD" pad="31"/>
<connect gate="G$1" pin="AVDD@1" pad="41"/>
<connect gate="G$1" pin="AVDD@2" pad="44"/>
<connect gate="G$1" pin="AVDD@3" pad="50"/>
<connect gate="G$1" pin="DGND" pad="56"/>
<connect gate="G$1" pin="DVDD" pad="4"/>
<connect gate="G$1" pin="DVDD@1" pad="17"/>
<connect gate="G$1" pin="GNDD" pad="16"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="26"/>
<connect gate="G$1" pin="PLLIN" pad="52"/>
<connect gate="G$1" pin="PLLOUT" pad="51"/>
<connect gate="G$1" pin="REFN" pad="40"/>
<connect gate="G$1" pin="REFP" pad="38"/>
<connect gate="G$1" pin="RXD0" pad="10"/>
<connect gate="G$1" pin="RXD1" pad="11"/>
<connect gate="G$1" pin="RXD10" pad="22"/>
<connect gate="G$1" pin="RXD11" pad="23"/>
<connect gate="G$1" pin="RXD12" pad="24"/>
<connect gate="G$1" pin="RXD13" pad="25"/>
<connect gate="G$1" pin="RXD2" pad="12"/>
<connect gate="G$1" pin="RXD3" pad="13"/>
<connect gate="G$1" pin="RXD4" pad="14"/>
<connect gate="G$1" pin="RXD5" pad="15"/>
<connect gate="G$1" pin="RXD6" pad="18"/>
<connect gate="G$1" pin="RXD7" pad="19"/>
<connect gate="G$1" pin="RXD8" pad="20"/>
<connect gate="G$1" pin="RXD9" pad="21"/>
<connect gate="G$1" pin="RXGAIN0" pad="28"/>
<connect gate="G$1" pin="RXGAIN1" pad="29"/>
<connect gate="G$1" pin="RXHYB+" pad="33"/>
<connect gate="G$1" pin="RXHYB-" pad="32"/>
<connect gate="G$1" pin="RXLINE+" pad="35"/>
<connect gate="G$1" pin="RXLINE-" pad="34"/>
<connect gate="G$1" pin="RXLOOP" pad="30"/>
<connect gate="G$1" pin="RXSYNC" pad="27"/>
<connect gate="G$1" pin="TXCLK" pad="7"/>
<connect gate="G$1" pin="TXDATA" pad="9"/>
<connect gate="G$1" pin="TXLINE+" pad="45"/>
<connect gate="G$1" pin="TXLINE-" pad="43"/>
<connect gate="G$1" pin="TXSCLK" pad="8"/>
<connect gate="G$1" pin="VCCLK" pad="3"/>
<connect gate="G$1" pin="VCDAC" pad="47"/>
<connect gate="G$1" pin="VCDATA" pad="54"/>
<connect gate="G$1" pin="VCINP" pad="2"/>
<connect gate="G$1" pin="VCLATCH" pad="53"/>
<connect gate="G$1" pin="VCM" pad="39"/>
<connect gate="G$1" pin="VCOUT" pad="1"/>
<connect gate="G$1" pin="VCSCLK" pad="55"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AFE1104" prefix="IC">
<description>&lt;b&gt;HDSL/MDSL Analog Front End&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AFE1104"/>
</gates>
<devices>
<device name="E" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="AGND" pad="32"/>
<connect gate="G$1" pin="AGND@1" pad="33"/>
<connect gate="G$1" pin="AGND@2" pad="38"/>
<connect gate="G$1" pin="AGND@3" pad="42"/>
<connect gate="G$1" pin="AV" pad="27"/>
<connect gate="G$1" pin="AV@1" pad="37"/>
<connect gate="G$1" pin="AV@2" pad="40"/>
<connect gate="G$1" pin="D0" pad="6"/>
<connect gate="G$1" pin="D1" pad="7"/>
<connect gate="G$1" pin="D10" pad="18"/>
<connect gate="G$1" pin="D11" pad="19"/>
<connect gate="G$1" pin="D12" pad="20"/>
<connect gate="G$1" pin="D13" pad="21"/>
<connect gate="G$1" pin="D2" pad="8"/>
<connect gate="G$1" pin="D3" pad="9"/>
<connect gate="G$1" pin="D4" pad="10"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="14"/>
<connect gate="G$1" pin="D7" pad="15"/>
<connect gate="G$1" pin="D8" pad="16"/>
<connect gate="G$1" pin="D9" pad="17"/>
<connect gate="G$1" pin="DGND" pad="4"/>
<connect gate="G$1" pin="DGND@1" pad="12"/>
<connect gate="G$1" pin="DV" pad="13"/>
<connect gate="G$1" pin="LINEN" pad="39"/>
<connect gate="G$1" pin="LINEP" pad="41"/>
<connect gate="G$1" pin="NC" pad="43"/>
<connect gate="G$1" pin="NC@1" pad="44"/>
<connect gate="G$1" pin="NC@2" pad="45"/>
<connect gate="G$1" pin="NC@3" pad="46"/>
<connect gate="G$1" pin="PGND" pad="1"/>
<connect gate="G$1" pin="PLLIN" pad="48"/>
<connect gate="G$1" pin="PLLOUT" pad="47"/>
<connect gate="G$1" pin="PV" pad="2"/>
<connect gate="G$1" pin="REFN" pad="36"/>
<connect gate="G$1" pin="REFP" pad="34"/>
<connect gate="G$1" pin="RXCLK" pad="22"/>
<connect gate="G$1" pin="RXGAIN0" pad="24"/>
<connect gate="G$1" pin="RXGAIN1" pad="25"/>
<connect gate="G$1" pin="RXHYBN" pad="28"/>
<connect gate="G$1" pin="RXHYBP" pad="29"/>
<connect gate="G$1" pin="RXLN" pad="30"/>
<connect gate="G$1" pin="RXLOOP" pad="26"/>
<connect gate="G$1" pin="RXLP" pad="31"/>
<connect gate="G$1" pin="RXSYNC" pad="23"/>
<connect gate="G$1" pin="TXCLK" pad="3"/>
<connect gate="G$1" pin="TXDAT" pad="5"/>
<connect gate="G$1" pin="VCM" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="AFE1104E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="74C7272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC4814" prefix="IC">
<description>&lt;b&gt;Quad 12-Bit DAC&lt;/b&gt;&lt;p&gt;
Serial Interface</description>
<gates>
<gate name="G$1" symbol="DAC4814"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!CLK" pad="19"/>
<connect gate="G$1" pin="!CLR" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="!LATCHA" pad="27"/>
<connect gate="G$1" pin="!LATCHB" pad="26"/>
<connect gate="G$1" pin="!LATCHC" pad="21"/>
<connect gate="G$1" pin="!LATCHD" pad="20"/>
<connect gate="G$1" pin="+VL" pad="28"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="-VS" pad="7"/>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="BPOA" pad="6"/>
<connect gate="G$1" pin="BPOB" pad="5"/>
<connect gate="G$1" pin="BPOC" pad="9"/>
<connect gate="G$1" pin="BPOD" pad="8"/>
<connect gate="G$1" pin="DATAIN" pad="22"/>
<connect gate="G$1" pin="DATAOUT" pad="18"/>
<connect gate="G$1" pin="DGND" pad="17"/>
<connect gate="G$1" pin="INVIN" pad="3"/>
<connect gate="G$1" pin="INVOUT" pad="11"/>
<connect gate="G$1" pin="MODE" pad="25"/>
<connect gate="G$1" pin="NC" pad="16"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="1"/>
<connect gate="G$1" pin="OUTC" pad="14"/>
<connect gate="G$1" pin="OUTD" pad="13"/>
<connect gate="G$1" pin="REFIN" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC4815P" prefix="IC">
<description>&lt;b&gt;Quad 12-Bit DAC&lt;/b&gt;&lt;p&gt;
8-Bit Port Interface</description>
<gates>
<gate name="G$1" symbol="DAC4815"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!CLR" pad="14"/>
<connect gate="G$1" pin="!CS" pad="16"/>
<connect gate="G$1" pin="!LE" pad="17"/>
<connect gate="G$1" pin="!WR" pad="15"/>
<connect gate="G$1" pin="+VL" pad="11"/>
<connect gate="G$1" pin="+VS" pad="8"/>
<connect gate="G$1" pin="-VS" pad="7"/>
<connect gate="G$1" pin="A0" pad="26"/>
<connect gate="G$1" pin="A1" pad="27"/>
<connect gate="G$1" pin="A2" pad="28"/>
<connect gate="G$1" pin="AGND" pad="9"/>
<connect gate="G$1" pin="BPO" pad="6"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="19"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="21"/>
<connect gate="G$1" pin="D4" pad="22"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="24"/>
<connect gate="G$1" pin="D7" pad="25"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="1"/>
<connect gate="G$1" pin="OUTC" pad="13"/>
<connect gate="G$1" pin="OUTD" pad="12"/>
<connect gate="G$1" pin="REF+" pad="5"/>
<connect gate="G$1" pin="REF-" pad="3"/>
<connect gate="G$1" pin="REFIN" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7819" prefix="IC">
<description>&lt;b&gt;12-Bit 800kHz Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7819"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="25"/>
<connect gate="G$1" pin="!CS" pad="24"/>
<connect gate="G$1" pin="+VANA" pad="20"/>
<connect gate="G$1" pin="+VANA@1" pad="28"/>
<connect gate="G$1" pin="+VDIG" pad="21"/>
<connect gate="G$1" pin="+VDIG@1" pad="27"/>
<connect gate="G$1" pin="-VANA" pad="26"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="7"/>
<connect gate="G$1" pin="D11" pad="6"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="D8" pad="9"/>
<connect gate="G$1" pin="D9" pad="8"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="NC" pad="19"/>
<connect gate="G$1" pin="R/!C" pad="23"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="25"/>
<connect gate="G$1" pin="!CS" pad="24"/>
<connect gate="G$1" pin="+VANA" pad="20"/>
<connect gate="G$1" pin="+VANA@1" pad="28"/>
<connect gate="G$1" pin="+VDIG" pad="21"/>
<connect gate="G$1" pin="+VDIG@1" pad="27"/>
<connect gate="G$1" pin="-VANA" pad="26"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="7"/>
<connect gate="G$1" pin="D11" pad="6"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="D8" pad="9"/>
<connect gate="G$1" pin="D9" pad="8"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="NC" pad="19"/>
<connect gate="G$1" pin="R/!C" pad="23"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7824" prefix="IC">
<description>&lt;b&gt;4-Channel, 12-Bit Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7824"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="A0" pad="19"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="AGND1" pad="1"/>
<connect gate="G$1" pin="AGND2" pad="8"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="4"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="21"/>
<connect gate="G$1" pin="CAP" pad="6"/>
<connect gate="G$1" pin="CONTC" pad="25"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="PAR/!SER" pad="20"/>
<connect gate="G$1" pin="PWRD" pad="26"/>
<connect gate="G$1" pin="R/!C" pad="22"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="VS1" pad="28"/>
<connect gate="G$1" pin="VS2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7824U"/>
<attribute name="OC_FARNELL" value="1106198"/>
<attribute name="OC_NEWARK" value="35C1550"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="A0" pad="19"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="AGND1" pad="1"/>
<connect gate="G$1" pin="AGND2" pad="8"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="4"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="21"/>
<connect gate="G$1" pin="CAP" pad="6"/>
<connect gate="G$1" pin="CONTC" pad="25"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="PAR/!SER" pad="20"/>
<connect gate="G$1" pin="PWRD" pad="26"/>
<connect gate="G$1" pin="R/!C" pad="22"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="VS1" pad="28"/>
<connect gate="G$1" pin="VS2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS7824P"/>
<attribute name="OC_FARNELL" value="1648604"/>
<attribute name="OC_NEWARK" value="14M8149"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7825" prefix="IC">
<description>&lt;b&gt;4 Channel, 16-Bit Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7824"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="A0" pad="19"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="AGND1" pad="1"/>
<connect gate="G$1" pin="AGND2" pad="8"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="4"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="21"/>
<connect gate="G$1" pin="CAP" pad="6"/>
<connect gate="G$1" pin="CONTC" pad="25"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="PAR/!SER" pad="20"/>
<connect gate="G$1" pin="PWRD" pad="26"/>
<connect gate="G$1" pin="R/!C" pad="22"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="VS1" pad="28"/>
<connect gate="G$1" pin="VS2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7825U"/>
<attribute name="OC_FARNELL" value="1097512"/>
<attribute name="OC_NEWARK" value="14M8151"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="A0" pad="19"/>
<connect gate="G$1" pin="A1" pad="18"/>
<connect gate="G$1" pin="AGND1" pad="1"/>
<connect gate="G$1" pin="AGND2" pad="8"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="4"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="BYTE" pad="21"/>
<connect gate="G$1" pin="CAP" pad="6"/>
<connect gate="G$1" pin="CONTC" pad="25"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="PAR/!SER" pad="20"/>
<connect gate="G$1" pin="PWRD" pad="26"/>
<connect gate="G$1" pin="R/!C" pad="22"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="VS1" pad="28"/>
<connect gate="G$1" pin="VS2" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7825P"/>
<attribute name="OC_FARNELL" value="1459283"/>
<attribute name="OC_NEWARK" value="14M8150"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7810" prefix="IC">
<description>&lt;b&gt;12-Bit 800kHz Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7819"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="25"/>
<connect gate="G$1" pin="!CS" pad="24"/>
<connect gate="G$1" pin="+VANA" pad="20"/>
<connect gate="G$1" pin="+VANA@1" pad="28"/>
<connect gate="G$1" pin="+VDIG" pad="21"/>
<connect gate="G$1" pin="+VDIG@1" pad="27"/>
<connect gate="G$1" pin="-VANA" pad="26"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="7"/>
<connect gate="G$1" pin="D11" pad="6"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="D8" pad="9"/>
<connect gate="G$1" pin="D9" pad="8"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="NC" pad="19"/>
<connect gate="G$1" pin="R/!C" pad="23"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7810U"/>
<attribute name="OC_FARNELL" value="1509511"/>
<attribute name="OC_NEWARK" value="73C9220"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="25"/>
<connect gate="G$1" pin="!CS" pad="24"/>
<connect gate="G$1" pin="+VANA" pad="20"/>
<connect gate="G$1" pin="+VANA@1" pad="28"/>
<connect gate="G$1" pin="+VDIG" pad="21"/>
<connect gate="G$1" pin="+VDIG@1" pad="27"/>
<connect gate="G$1" pin="-VANA" pad="26"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="7"/>
<connect gate="G$1" pin="D11" pad="6"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="D8" pad="9"/>
<connect gate="G$1" pin="D9" pad="8"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="NC" pad="19"/>
<connect gate="G$1" pin="R/!C" pad="23"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7833N" prefix="IC">
<description>&lt;b&gt;10-Channel, 12-Bit Data Acquisition System&lt;/b&gt;&lt;p&gt;
three synchronized A/D converters and seven S/H amplifiers</description>
<gates>
<gate name="G$1" symbol="ADS7833"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="AGND" pad="67"/>
<connect gate="G$1" pin="AOUT" pad="62"/>
<connect gate="G$1" pin="ASH" pad="38"/>
<connect gate="G$1" pin="BUSY" pad="40"/>
<connect gate="G$1" pin="CLK" pad="36"/>
<connect gate="G$1" pin="CONV" pad="37"/>
<connect gate="G$1" pin="DCLOCK" pad="41"/>
<connect gate="G$1" pin="DGND" pad="30"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC@1" pad="10"/>
<connect gate="G$1" pin="NC@10" pad="25"/>
<connect gate="G$1" pin="NC@11" pad="26"/>
<connect gate="G$1" pin="NC@12" pad="32"/>
<connect gate="G$1" pin="NC@13" pad="42"/>
<connect gate="G$1" pin="NC@14" pad="43"/>
<connect gate="G$1" pin="NC@15" pad="44"/>
<connect gate="G$1" pin="NC@16" pad="45"/>
<connect gate="G$1" pin="NC@17" pad="46"/>
<connect gate="G$1" pin="NC@18" pad="47"/>
<connect gate="G$1" pin="NC@19" pad="48"/>
<connect gate="G$1" pin="NC@2" pad="13"/>
<connect gate="G$1" pin="NC@20" pad="49"/>
<connect gate="G$1" pin="NC@21" pad="50"/>
<connect gate="G$1" pin="NC@22" pad="51"/>
<connect gate="G$1" pin="NC@23" pad="54"/>
<connect gate="G$1" pin="NC@24" pad="57"/>
<connect gate="G$1" pin="NC@25" pad="60"/>
<connect gate="G$1" pin="NC@26" pad="61"/>
<connect gate="G$1" pin="NC@3" pad="16"/>
<connect gate="G$1" pin="NC@4" pad="19"/>
<connect gate="G$1" pin="NC@5" pad="20"/>
<connect gate="G$1" pin="NC@6" pad="21"/>
<connect gate="G$1" pin="NC@7" pad="22"/>
<connect gate="G$1" pin="NC@8" pad="23"/>
<connect gate="G$1" pin="NC@9" pad="24"/>
<connect gate="G$1" pin="REFGND" pad="65"/>
<connect gate="G$1" pin="REFIN" pad="64"/>
<connect gate="G$1" pin="REFOUT" pad="63"/>
<connect gate="G$1" pin="SERIN" pad="39"/>
<connect gate="G$1" pin="SOUT1" pad="35"/>
<connect gate="G$1" pin="SOUT2" pad="33"/>
<connect gate="G$1" pin="SOUT3" pad="34"/>
<connect gate="G$1" pin="TP1" pad="27"/>
<connect gate="G$1" pin="TP2" pad="28"/>
<connect gate="G$1" pin="V1-1N" pad="59"/>
<connect gate="G$1" pin="V1-1P" pad="58"/>
<connect gate="G$1" pin="V1-2N" pad="56"/>
<connect gate="G$1" pin="V1-2P" pad="55"/>
<connect gate="G$1" pin="V1-3N" pad="53"/>
<connect gate="G$1" pin="V1-3P" pad="52"/>
<connect gate="G$1" pin="V2-1N" pad="11"/>
<connect gate="G$1" pin="V2-1P" pad="12"/>
<connect gate="G$1" pin="V2-2N" pad="14"/>
<connect gate="G$1" pin="V2-2P" pad="15"/>
<connect gate="G$1" pin="V2-3N" pad="17"/>
<connect gate="G$1" pin="V2-3P" pad="18"/>
<connect gate="G$1" pin="V3-1N" pad="8"/>
<connect gate="G$1" pin="V3-1P" pad="9"/>
<connect gate="G$1" pin="V3-2N" pad="5"/>
<connect gate="G$1" pin="V3-2P" pad="6"/>
<connect gate="G$1" pin="V3-3N" pad="3"/>
<connect gate="G$1" pin="V3-3P" pad="4"/>
<connect gate="G$1" pin="V3-4N" pad="1"/>
<connect gate="G$1" pin="V3-4P" pad="2"/>
<connect gate="G$1" pin="VANA+" pad="68"/>
<connect gate="G$1" pin="VANA-" pad="66"/>
<connect gate="G$1" pin="VDIG+" pad="29"/>
<connect gate="G$1" pin="VDIG-" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS800" prefix="IC">
<description>&lt;b&gt;1-Bit, 40 MSPS ADC SE/Diff inputs&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS800"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B11" pad="12"/>
<connect gate="G$1" pin="B12" pad="13"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B11" pad="12"/>
<connect gate="G$1" pin="B12" pad="13"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS800U"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="35C1569"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7831" prefix="IC">
<description>&lt;b&gt;12-Bit 600kHz Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7819"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="25"/>
<connect gate="G$1" pin="!CS" pad="24"/>
<connect gate="G$1" pin="+VANA" pad="20"/>
<connect gate="G$1" pin="+VANA@1" pad="28"/>
<connect gate="G$1" pin="+VDIG" pad="21"/>
<connect gate="G$1" pin="+VDIG@1" pad="27"/>
<connect gate="G$1" pin="-VANA" pad="26"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="7"/>
<connect gate="G$1" pin="D11" pad="6"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="D8" pad="9"/>
<connect gate="G$1" pin="D9" pad="8"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="NC" pad="19"/>
<connect gate="G$1" pin="R/!C" pad="23"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="25"/>
<connect gate="G$1" pin="!CS" pad="24"/>
<connect gate="G$1" pin="+VANA" pad="20"/>
<connect gate="G$1" pin="+VANA@1" pad="28"/>
<connect gate="G$1" pin="+VDIG" pad="21"/>
<connect gate="G$1" pin="+VDIG@1" pad="27"/>
<connect gate="G$1" pin="-VANA" pad="26"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="7"/>
<connect gate="G$1" pin="D11" pad="6"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="D8" pad="9"/>
<connect gate="G$1" pin="D9" pad="8"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="NC" pad="19"/>
<connect gate="G$1" pin="R/!C" pad="23"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7817" prefix="IC">
<description>&lt;b&gt;12-Bit Diff. Input Micro Power Sampling ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7817"/>
</gates>
<devices>
<device name="E" package="MSOP08">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="DCLOCK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS7817E/250G4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="73K7081"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="DCLOCK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08-GW">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="DCLOCK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS7817UC"/>
<attribute name="OC_FARNELL" value="1407035"/>
<attribute name="OC_NEWARK" value="74C7126"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7816" prefix="IC">
<description>&lt;b&gt;12-Bit High Speed Micro Power Sampling ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7817"/>
</gates>
<devices>
<device name="E" package="MSOP08">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="DCLOCK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS7816EC/250"/>
<attribute name="OC_FARNELL" value="1754724"/>
<attribute name="OC_NEWARK" value="74C7108"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="DCLOCK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS7816P"/>
<attribute name="OC_FARNELL" value="1097576"/>
<attribute name="OC_NEWARK" value="14M9332"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08-GW">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="DCLOCK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7816U"/>
<attribute name="OC_FARNELL" value="1273124"/>
<attribute name="OC_NEWARK" value="80K5554"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7806" prefix="IC">
<description>&lt;b&gt;Low-Power 12-Bit Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7806"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="6"/>
<connect gate="G$1" pin="BYTE" pad="21"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DATACLK" pad="18"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="EXT/!INT" pad="8"/>
<connect gate="G$1" pin="PWRD" pad="25"/>
<connect gate="G$1" pin="R/!C" pad="22"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="REFD" pad="26"/>
<connect gate="G$1" pin="SB/!PTC" pad="7"/>
<connect gate="G$1" pin="SDATA" pad="19"/>
<connect gate="G$1" pin="TAG" pad="20"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1106202"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="6"/>
<connect gate="G$1" pin="BYTE" pad="21"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DATACLK" pad="18"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="EXT/!INT" pad="8"/>
<connect gate="G$1" pin="PWRD" pad="25"/>
<connect gate="G$1" pin="R/!C" pad="22"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="REFD" pad="26"/>
<connect gate="G$1" pin="SB/!PTC" pad="7"/>
<connect gate="G$1" pin="SDATA" pad="19"/>
<connect gate="G$1" pin="TAG" pad="20"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS7806PG4"/>
<attribute name="OC_FARNELL" value="1178440"/>
<attribute name="OC_NEWARK" value="81K0043"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7807" prefix="IC">
<description>&lt;b&gt;Low-Power 16-Bit Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7806"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="6"/>
<connect gate="G$1" pin="BYTE" pad="21"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DATACLK" pad="18"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="EXT/!INT" pad="8"/>
<connect gate="G$1" pin="PWRD" pad="25"/>
<connect gate="G$1" pin="R/!C" pad="22"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="REFD" pad="26"/>
<connect gate="G$1" pin="SB/!PTC" pad="7"/>
<connect gate="G$1" pin="SDATA" pad="19"/>
<connect gate="G$1" pin="TAG" pad="20"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7807U"/>
<attribute name="OC_FARNELL" value="1273123"/>
<attribute name="OC_NEWARK" value="80K5548"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="24"/>
<connect gate="G$1" pin="!CS" pad="23"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="6"/>
<connect gate="G$1" pin="BYTE" pad="21"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="13"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="DATACLK" pad="18"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="EXT/!INT" pad="8"/>
<connect gate="G$1" pin="PWRD" pad="25"/>
<connect gate="G$1" pin="R/!C" pad="22"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="REFD" pad="26"/>
<connect gate="G$1" pin="SB/!PTC" pad="7"/>
<connect gate="G$1" pin="SDATA" pad="19"/>
<connect gate="G$1" pin="TAG" pad="20"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7807P"/>
<attribute name="OC_FARNELL" value="1097549"/>
<attribute name="OC_NEWARK" value="74C7075"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7809" prefix="IC">
<description>&lt;b&gt;16-Bit 10us Serial CMOS Sampling ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7809"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="!BUSY" pad="17"/>
<connect gate="G$1" pin="!CS" pad="16"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="7"/>
<connect gate="G$1" pin="CAP" pad="5"/>
<connect gate="G$1" pin="DATA" pad="13"/>
<connect gate="G$1" pin="DATACLK" pad="12"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="EXT/!INT" pad="9"/>
<connect gate="G$1" pin="PWRD" pad="18"/>
<connect gate="G$1" pin="R/!C" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="R3IN" pad="4"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="SB/!BTC" pad="8"/>
<connect gate="G$1" pin="SYNC" pad="11"/>
<connect gate="G$1" pin="TAG" pad="14"/>
<connect gate="G$1" pin="VANA" pad="19"/>
<connect gate="G$1" pin="VDIG" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD977ANZ"/>
<attribute name="OC_FARNELL" value="1079312"/>
<attribute name="OC_NEWARK" value="59K7418"/>
</technology>
</technologies>
</device>
<device name="U" package="SO20L">
<connects>
<connect gate="G$1" pin="!BUSY" pad="17"/>
<connect gate="G$1" pin="!CS" pad="16"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="7"/>
<connect gate="G$1" pin="CAP" pad="5"/>
<connect gate="G$1" pin="DATA" pad="13"/>
<connect gate="G$1" pin="DATACLK" pad="12"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="EXT/!INT" pad="9"/>
<connect gate="G$1" pin="PWRD" pad="18"/>
<connect gate="G$1" pin="R/!C" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="R3IN" pad="4"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="SB/!BTC" pad="8"/>
<connect gate="G$1" pin="SYNC" pad="11"/>
<connect gate="G$1" pin="TAG" pad="14"/>
<connect gate="G$1" pin="VANA" pad="19"/>
<connect gate="G$1" pin="VDIG" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7809U"/>
<attribute name="OC_FARNELL" value="1214386"/>
<attribute name="OC_NEWARK" value="80K5549"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7813" prefix="IC">
<description>&lt;b&gt;Low-Power, Serial 16-Bit Sampling ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7812"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!BUSY" pad="14"/>
<connect gate="G$1" pin="!CONV" pad="12"/>
<connect gate="G$1" pin="!CS" pad="13"/>
<connect gate="G$1" pin="BUF" pad="5"/>
<connect gate="G$1" pin="CAP" pad="6"/>
<connect gate="G$1" pin="DATA" pad="10"/>
<connect gate="G$1" pin="DATACLK" pad="9"/>
<connect gate="G$1" pin="EXT/!INT" pad="11"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PWRD" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="R3IN" pad="4"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="VS" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS7813P"/>
<attribute name="OC_FARNELL" value="1212285"/>
<attribute name="OC_NEWARK" value="01M6818"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="!BUSY" pad="14"/>
<connect gate="G$1" pin="!CONV" pad="12"/>
<connect gate="G$1" pin="!CS" pad="13"/>
<connect gate="G$1" pin="BUF" pad="5"/>
<connect gate="G$1" pin="CAP" pad="6"/>
<connect gate="G$1" pin="DATA" pad="10"/>
<connect gate="G$1" pin="DATACLK" pad="9"/>
<connect gate="G$1" pin="EXT/!INT" pad="11"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="PWRD" pad="15"/>
<connect gate="G$1" pin="R1IN" pad="1"/>
<connect gate="G$1" pin="R2IN" pad="3"/>
<connect gate="G$1" pin="R3IN" pad="4"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="VS" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7813U"/>
<attribute name="OC_FARNELL" value="1459277"/>
<attribute name="OC_NEWARK" value="80K5551"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7815" prefix="IC">
<description>&lt;b&gt;16-Bit 250kHz Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7815"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="26"/>
<connect gate="G$1" pin="!CS" pad="25"/>
<connect gate="G$1" pin="+VS" pad="27"/>
<connect gate="G$1" pin="+VS@1" pad="28"/>
<connect gate="G$1" pin="-VS" pad="23"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="D0" pad="22"/>
<connect gate="G$1" pin="D1" pad="21"/>
<connect gate="G$1" pin="D10" pad="11"/>
<connect gate="G$1" pin="D11" pad="10"/>
<connect gate="G$1" pin="D12" pad="9"/>
<connect gate="G$1" pin="D13" pad="8"/>
<connect gate="G$1" pin="D14" pad="7"/>
<connect gate="G$1" pin="D15" pad="6"/>
<connect gate="G$1" pin="D2" pad="20"/>
<connect gate="G$1" pin="D3" pad="19"/>
<connect gate="G$1" pin="D4" pad="18"/>
<connect gate="G$1" pin="D5" pad="17"/>
<connect gate="G$1" pin="D6" pad="16"/>
<connect gate="G$1" pin="D7" pad="15"/>
<connect gate="G$1" pin="D8" pad="13"/>
<connect gate="G$1" pin="D9" pad="12"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="R/!C" pad="24"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS7815UE4"/>
<attribute name="OC_FARNELL" value="1206867"/>
<attribute name="OC_NEWARK" value="96K6229"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1212" prefix="IC">
<description>&lt;b&gt;22-Bit Analog-to-Digital Converter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS1212"/>
</gates>
<devices>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="!CS" pad="5"/>
<connect gate="G$1" pin="!DRDY" pad="14"/>
<connect gate="G$1" pin="!DSYNC" pad="6"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AINN" pad="2"/>
<connect gate="G$1" pin="AINP" pad="1"/>
<connect gate="G$1" pin="AVDD" pad="16"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DVDD" pad="10"/>
<connect gate="G$1" pin="MODE" pad="15"/>
<connect gate="G$1" pin="REFIN" pad="18"/>
<connect gate="G$1" pin="REFOUT" pad="17"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDIO" pad="12"/>
<connect gate="G$1" pin="SDOUT" pad="13"/>
<connect gate="G$1" pin="VBIAS" pad="4"/>
<connect gate="G$1" pin="XIN" pad="7"/>
<connect gate="G$1" pin="XOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS1212P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K4581"/>
</technology>
</technologies>
</device>
<device name="U" package="SO18L">
<connects>
<connect gate="G$1" pin="!CS" pad="5"/>
<connect gate="G$1" pin="!DRDY" pad="14"/>
<connect gate="G$1" pin="!DSYNC" pad="6"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AINN" pad="2"/>
<connect gate="G$1" pin="AINP" pad="1"/>
<connect gate="G$1" pin="AVDD" pad="16"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DVDD" pad="10"/>
<connect gate="G$1" pin="MODE" pad="15"/>
<connect gate="G$1" pin="REFIN" pad="18"/>
<connect gate="G$1" pin="REFOUT" pad="17"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDIO" pad="12"/>
<connect gate="G$1" pin="SDOUT" pad="13"/>
<connect gate="G$1" pin="VBIAS" pad="4"/>
<connect gate="G$1" pin="XIN" pad="7"/>
<connect gate="G$1" pin="XOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS1212U"/>
<attribute name="OC_FARNELL" value="1459252"/>
<attribute name="OC_NEWARK" value="61M4770"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1213" prefix="IC">
<description>&lt;b&gt;22-Bit Analog-to-Digital Converter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS1213"/>
</gates>
<devices>
<device name="P" package="DIL24-3">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="!DRDY" pad="17"/>
<connect gate="G$1" pin="!DSYNC" pad="9"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="24"/>
<connect gate="G$1" pin="AIN4N" pad="23"/>
<connect gate="G$1" pin="AIN4P" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="MODE" pad="18"/>
<connect gate="G$1" pin="REFIN" pad="21"/>
<connect gate="G$1" pin="REFOUT" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="SDIO" pad="15"/>
<connect gate="G$1" pin="SDOUT" pad="16"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="10"/>
<connect gate="G$1" pin="XOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1213P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="14M9330"/>
</technology>
</technologies>
</device>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!CS" pad="10"/>
<connect gate="G$1" pin="!DRDY" pad="19"/>
<connect gate="G$1" pin="!DSYNC" pad="11"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="28"/>
<connect gate="G$1" pin="AIN4N" pad="27"/>
<connect gate="G$1" pin="AIN4P" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="23"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="MODE" pad="22"/>
<connect gate="G$1" pin="REFIN" pad="25"/>
<connect gate="G$1" pin="REFOUT" pad="24"/>
<connect gate="G$1" pin="SCLK" pad="16"/>
<connect gate="G$1" pin="SDIO" pad="17"/>
<connect gate="G$1" pin="SDOUT" pad="18"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="12"/>
<connect gate="G$1" pin="XOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1213E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="74C6980"/>
</technology>
</technologies>
</device>
<device name="U" package="SO24L">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="!DRDY" pad="17"/>
<connect gate="G$1" pin="!DSYNC" pad="9"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="24"/>
<connect gate="G$1" pin="AIN4N" pad="23"/>
<connect gate="G$1" pin="AIN4P" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="MODE" pad="18"/>
<connect gate="G$1" pin="REFIN" pad="21"/>
<connect gate="G$1" pin="REFOUT" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="SDIO" pad="15"/>
<connect gate="G$1" pin="SDOUT" pad="16"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="10"/>
<connect gate="G$1" pin="XOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1213U"/>
<attribute name="OC_FARNELL" value="1234905"/>
<attribute name="OC_NEWARK" value="35C1517"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1210" prefix="IC">
<description>&lt;b&gt;24-Bit Analog-to-Digital Converter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS1212"/>
</gates>
<devices>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="!CS" pad="5"/>
<connect gate="G$1" pin="!DRDY" pad="14"/>
<connect gate="G$1" pin="!DSYNC" pad="6"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AINN" pad="2"/>
<connect gate="G$1" pin="AINP" pad="1"/>
<connect gate="G$1" pin="AVDD" pad="16"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DVDD" pad="10"/>
<connect gate="G$1" pin="MODE" pad="15"/>
<connect gate="G$1" pin="REFIN" pad="18"/>
<connect gate="G$1" pin="REFOUT" pad="17"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDIO" pad="12"/>
<connect gate="G$1" pin="SDOUT" pad="13"/>
<connect gate="G$1" pin="VBIAS" pad="4"/>
<connect gate="G$1" pin="XIN" pad="7"/>
<connect gate="G$1" pin="XOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1210P"/>
<attribute name="OC_FARNELL" value="1312336"/>
<attribute name="OC_NEWARK" value="96K4580"/>
</technology>
</technologies>
</device>
<device name="U" package="SO18L">
<connects>
<connect gate="G$1" pin="!CS" pad="5"/>
<connect gate="G$1" pin="!DRDY" pad="14"/>
<connect gate="G$1" pin="!DSYNC" pad="6"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AINN" pad="2"/>
<connect gate="G$1" pin="AINP" pad="1"/>
<connect gate="G$1" pin="AVDD" pad="16"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DVDD" pad="10"/>
<connect gate="G$1" pin="MODE" pad="15"/>
<connect gate="G$1" pin="REFIN" pad="18"/>
<connect gate="G$1" pin="REFOUT" pad="17"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDIO" pad="12"/>
<connect gate="G$1" pin="SDOUT" pad="13"/>
<connect gate="G$1" pin="VBIAS" pad="4"/>
<connect gate="G$1" pin="XIN" pad="7"/>
<connect gate="G$1" pin="XOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1210U"/>
<attribute name="OC_FARNELL" value="1097511"/>
<attribute name="OC_NEWARK" value="74K3627"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1211" prefix="IC">
<description>&lt;b&gt;24-Bit Analog-to-Digital Converter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS1211"/>
</gates>
<devices>
<device name="P" package="DIL24-3">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="!DRDY" pad="17"/>
<connect gate="G$1" pin="!DSYNC" pad="9"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="24"/>
<connect gate="G$1" pin="AIN4N" pad="23"/>
<connect gate="G$1" pin="AIN4P" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="MODE" pad="18"/>
<connect gate="G$1" pin="REFIN" pad="21"/>
<connect gate="G$1" pin="REFOUT" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="SDIO" pad="15"/>
<connect gate="G$1" pin="SDOUT" pad="16"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="10"/>
<connect gate="G$1" pin="XOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1211P"/>
<attribute name="OC_FARNELL" value="1219430"/>
<attribute name="OC_NEWARK" value="96K2329"/>
</technology>
</technologies>
</device>
<device name="E" package="SSOP28DL">
<connects>
<connect gate="G$1" pin="!CS" pad="10"/>
<connect gate="G$1" pin="!DRDY" pad="19"/>
<connect gate="G$1" pin="!DSYNC" pad="11"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="28"/>
<connect gate="G$1" pin="AIN4N" pad="27"/>
<connect gate="G$1" pin="AIN4P" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="23"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="MODE" pad="22"/>
<connect gate="G$1" pin="REFIN" pad="25"/>
<connect gate="G$1" pin="REFOUT" pad="24"/>
<connect gate="G$1" pin="SCLK" pad="16"/>
<connect gate="G$1" pin="SDIO" pad="17"/>
<connect gate="G$1" pin="SDOUT" pad="18"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="12"/>
<connect gate="G$1" pin="XOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS1211E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="74C6976"/>
</technology>
</technologies>
</device>
<device name="U" package="SO24L">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="!DRDY" pad="17"/>
<connect gate="G$1" pin="!DSYNC" pad="9"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="24"/>
<connect gate="G$1" pin="AIN4N" pad="23"/>
<connect gate="G$1" pin="AIN4P" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="MODE" pad="18"/>
<connect gate="G$1" pin="REFIN" pad="21"/>
<connect gate="G$1" pin="REFOUT" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="SDIO" pad="15"/>
<connect gate="G$1" pin="SDOUT" pad="16"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="10"/>
<connect gate="G$1" pin="XOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="ADS1211U.."/>
<attribute name="OC_FARNELL" value="9324070"/>
<attribute name="OC_NEWARK" value="37K8944"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1286" prefix="IC">
<description>&lt;b&gt;12-Bit Micro Power Sampling ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7817"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="DCLOCK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS1286P"/>
<attribute name="OC_FARNELL" value="1214453"/>
<attribute name="OC_NEWARK" value="74C7011"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="!CS!/SHDN" pad="5"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="DCLOCK" pad="7"/>
<connect gate="G$1" pin="DOUT" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1286U"/>
<attribute name="OC_FARNELL" value="1106203"/>
<attribute name="OC_NEWARK" value="80K5544"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS931" prefix="IC">
<description>&lt;b&gt;8-Bit, 30 MSPS ADC SE/Diff Inputs&lt;/b&gt;&lt;p&gt;
External Ref. and Low; Power, Powerdown</description>
<gates>
<gate name="G$1" symbol="ADS931"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!OE" pad="16"/>
<connect gate="G$1" pin="+VS" pad="1"/>
<connect gate="G$1" pin="+VS@1" pad="18"/>
<connect gate="G$1" pin="+VS@2" pad="28"/>
<connect gate="G$1" pin="B1" pad="12"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="10"/>
<connect gate="G$1" pin="B4" pad="9"/>
<connect gate="G$1" pin="B5" pad="8"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="6"/>
<connect gate="G$1" pin="B8" pad="5"/>
<connect gate="G$1" pin="CLK" pad="15"/>
<connect gate="G$1" pin="CM" pad="26"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="IN" pad="27"/>
<connect gate="G$1" pin="LNBY" pad="25"/>
<connect gate="G$1" pin="LPBY" pad="21"/>
<connect gate="G$1" pin="LVDD" pad="2"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="23"/>
<connect gate="G$1" pin="PWRD" pad="17"/>
<connect gate="G$1" pin="REFB" pad="24"/>
<connect gate="G$1" pin="REFT" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS931E.."/>
<attribute name="OC_FARNELL" value="1648611"/>
<attribute name="OC_NEWARK" value="80P3665"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS930" prefix="IC">
<description>&lt;b&gt;8-Bit, 30 MSPS ADC SE/Diff Inputs&lt;/b&gt;&lt;p&gt;
Internal Ref. and Low Power, Powerdown</description>
<gates>
<gate name="G$1" symbol="ADS930"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="24"/>
<connect gate="G$1" pin="!OE" pad="16"/>
<connect gate="G$1" pin="+IN" pad="27"/>
<connect gate="G$1" pin="+VS" pad="1"/>
<connect gate="G$1" pin="+VS@1" pad="18"/>
<connect gate="G$1" pin="+VS@2" pad="28"/>
<connect gate="G$1" pin="1VREF" pad="23"/>
<connect gate="G$1" pin="B1" pad="12"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="10"/>
<connect gate="G$1" pin="B4" pad="9"/>
<connect gate="G$1" pin="B5" pad="8"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="6"/>
<connect gate="G$1" pin="B8" pad="5"/>
<connect gate="G$1" pin="CLK" pad="15"/>
<connect gate="G$1" pin="CM" pad="26"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="LNBY" pad="25"/>
<connect gate="G$1" pin="LPBY" pad="21"/>
<connect gate="G$1" pin="LVDD" pad="2"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="22"/>
<connect gate="G$1" pin="PWRD" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD9280ARSZ"/>
<attribute name="OC_FARNELL" value="9603727"/>
<attribute name="OC_NEWARK" value="19M1009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS902" prefix="IC">
<description>&lt;b&gt;10-Bit, 30 MSPS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS902"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!OE" pad="16"/>
<connect gate="G$1" pin="+VS" pad="1"/>
<connect gate="G$1" pin="+VS@1" pad="18"/>
<connect gate="G$1" pin="+VS@2" pad="28"/>
<connect gate="G$1" pin="B1" pad="12"/>
<connect gate="G$1" pin="B10" pad="3"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="10"/>
<connect gate="G$1" pin="B4" pad="9"/>
<connect gate="G$1" pin="B5" pad="8"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="6"/>
<connect gate="G$1" pin="B8" pad="5"/>
<connect gate="G$1" pin="B9" pad="4"/>
<connect gate="G$1" pin="CLK" pad="15"/>
<connect gate="G$1" pin="CM" pad="26"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="IN" pad="27"/>
<connect gate="G$1" pin="LNBY" pad="25"/>
<connect gate="G$1" pin="LPBY" pad="21"/>
<connect gate="G$1" pin="LVDD" pad="2"/>
<connect gate="G$1" pin="NC" pad="23"/>
<connect gate="G$1" pin="PWRD" pad="17"/>
<connect gate="G$1" pin="REFB" pad="24"/>
<connect gate="G$1" pin="REFT" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS900" prefix="IC">
<description>&lt;b&gt;10-Bit, 20 MSPS ADC SE/Diff Inputs&lt;/b&gt;&lt;p&gt;
Int Reference and Adjustable Fullscale Range</description>
<gates>
<gate name="G$1" symbol="ADS900"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="24"/>
<connect gate="G$1" pin="!OE" pad="16"/>
<connect gate="G$1" pin="+VS" pad="1"/>
<connect gate="G$1" pin="+VS@1" pad="18"/>
<connect gate="G$1" pin="+VS@2" pad="28"/>
<connect gate="G$1" pin="1VREF" pad="23"/>
<connect gate="G$1" pin="B1" pad="12"/>
<connect gate="G$1" pin="B10" pad="3"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="10"/>
<connect gate="G$1" pin="B4" pad="9"/>
<connect gate="G$1" pin="B5" pad="8"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="6"/>
<connect gate="G$1" pin="B8" pad="5"/>
<connect gate="G$1" pin="B9" pad="4"/>
<connect gate="G$1" pin="CLK" pad="15"/>
<connect gate="G$1" pin="CM" pad="26"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="IN" pad="27"/>
<connect gate="G$1" pin="LNBY" pad="25"/>
<connect gate="G$1" pin="LPBY" pad="21"/>
<connect gate="G$1" pin="LVDD" pad="2"/>
<connect gate="G$1" pin="NC" pad="22"/>
<connect gate="G$1" pin="PWRD" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS900E"/>
<attribute name="OC_FARNELL" value="1459301"/>
<attribute name="OC_NEWARK" value="74C7264"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS801" prefix="IC">
<description>&lt;b&gt;1-Bit, 25 MSPS ADC SE/Diff inputs&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS801"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B11" pad="12"/>
<connect gate="G$1" pin="B12" pad="13"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B11" pad="12"/>
<connect gate="G$1" pin="B12" pad="13"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS801U"/>
<attribute name="OC_FARNELL" value="4808320"/>
<attribute name="OC_NEWARK" value="35C1570"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS802" prefix="IC">
<description>&lt;b&gt;1-Bit, 10 MSPS ADC SE/Diff inputs&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS801"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B11" pad="12"/>
<connect gate="G$1" pin="B12" pad="13"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B11" pad="12"/>
<connect gate="G$1" pin="B12" pad="13"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS802U"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16C1136"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS820" prefix="IC">
<description>&lt;b&gt;10-Bit, 20 MSPS ADC SE/Diff Inputs&lt;/b&gt;&lt;p&gt;
with Int References and 9.5 bit ENOB</description>
<gates>
<gate name="G$1" symbol="ADS820"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS820U"/>
<attribute name="OC_FARNELL" value="1214452"/>
<attribute name="OC_NEWARK" value="74C7210"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS821" prefix="IC">
<description>&lt;b&gt;10-Bit, 40 MSPS ADC SE/Diff Inputs&lt;/b&gt;&lt;p&gt;
with Int References and 9.3 bit ENOB</description>
<gates>
<gate name="G$1" symbol="ADS820"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="25"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!IN" pad="27"/>
<connect gate="G$1" pin="!OE" pad="18"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="17"/>
<connect gate="G$1" pin="+VS@2" pad="20"/>
<connect gate="G$1" pin="+VS@3" pad="24"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="CM" pad="22"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="28"/>
<connect gate="G$1" pin="IN" pad="26"/>
<connect gate="G$1" pin="MSBI" pad="19"/>
<connect gate="G$1" pin="NC" pad="12"/>
<connect gate="G$1" pin="NC@1" pad="13"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="REFT" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS821U"/>
<attribute name="OC_FARNELL" value="1509519"/>
<attribute name="OC_NEWARK" value="35C1575"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS823" prefix="IC">
<description>&lt;b&gt;10-Bit, 60 MSPS ADC SE/Diff, Int/Ext Ref.&lt;/b&gt;&lt;p&gt;
program. i/p range  w/Pwrdown</description>
<gates>
<gate name="G$1" symbol="ADS823"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="24"/>
<connect gate="G$1" pin="!OE" pad="12"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="27"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="BYB" pad="20"/>
<connect gate="G$1" pin="BYT" pad="21"/>
<connect gate="G$1" pin="CLK" pad="14"/>
<connect gate="G$1" pin="CM" pad="23"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="26"/>
<connect gate="G$1" pin="IN" pad="25"/>
<connect gate="G$1" pin="INT/EXT" pad="18"/>
<connect gate="G$1" pin="PD" pad="13"/>
<connect gate="G$1" pin="REFB" pad="19"/>
<connect gate="G$1" pin="REFT" pad="22"/>
<connect gate="G$1" pin="RSEL" pad="17"/>
<connect gate="G$1" pin="VDRV" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS823E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="35C1576"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS824" prefix="IC">
<description>&lt;b&gt;10-Bit, 70 MSPS ADC SE/Diff, Int/Ext Ref.&lt;/b&gt;&lt;p&gt;
program. i/p range w/Pwrdown</description>
<gates>
<gate name="G$1" symbol="ADS823"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!IN" pad="24"/>
<connect gate="G$1" pin="!OE" pad="12"/>
<connect gate="G$1" pin="+VS" pad="15"/>
<connect gate="G$1" pin="+VS@1" pad="27"/>
<connect gate="G$1" pin="B1" pad="2"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B2" pad="3"/>
<connect gate="G$1" pin="B3" pad="4"/>
<connect gate="G$1" pin="B4" pad="5"/>
<connect gate="G$1" pin="B5" pad="6"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="8"/>
<connect gate="G$1" pin="B8" pad="9"/>
<connect gate="G$1" pin="B9" pad="10"/>
<connect gate="G$1" pin="BYB" pad="20"/>
<connect gate="G$1" pin="BYT" pad="21"/>
<connect gate="G$1" pin="CLK" pad="14"/>
<connect gate="G$1" pin="CM" pad="23"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="16"/>
<connect gate="G$1" pin="GND@2" pad="26"/>
<connect gate="G$1" pin="IN" pad="25"/>
<connect gate="G$1" pin="INT/EXT" pad="18"/>
<connect gate="G$1" pin="PD" pad="13"/>
<connect gate="G$1" pin="REFB" pad="19"/>
<connect gate="G$1" pin="REFT" pad="22"/>
<connect gate="G$1" pin="RSEL" pad="17"/>
<connect gate="G$1" pin="VDRV" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA124" prefix="IC">
<description>&lt;b&gt;Difet Operational Amplifier&lt;/b&gt;&lt;p&gt;
Low Noise, Precision</description>
<gates>
<gate name="G$1" symbol="2TRIMSUB"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="SUBS" pad="8"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA548" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
High-Voltage, High-Current</description>
<gates>
<gate name="G$1" symbol="OPA548"/>
</gates>
<devices>
<device name="F" package="DD-7">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="E/S" pad="7"/>
<connect gate="G$1" pin="ILIM" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA548FKTWTG3"/>
<attribute name="OC_FARNELL" value="1234750"/>
<attribute name="OC_NEWARK" value="80K2676"/>
</technology>
</technologies>
</device>
<device name="T" package="TO220-7">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="E/S" pad="7"/>
<connect gate="G$1" pin="ILIM" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA548T"/>
<attribute name="OC_FARNELL" value="1564885"/>
<attribute name="OC_NEWARK" value="69K2680"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2340" prefix="IC">
<description>&lt;b&gt;Single-Supply, Rail-to-Rail Operational Amplifiers&lt;/b&gt;&lt;p&gt;
MicroAmplifier(TM) Series; Product Folder:OPA2340</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="E" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2340EA/250"/>
<attribute name="OC_FARNELL" value="1101540"/>
<attribute name="OC_NEWARK" value="36K7580"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2340PA"/>
<attribute name="OC_FARNELL" value="1129252"/>
<attribute name="OC_NEWARK" value="62K3460"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2340UA"/>
<attribute name="OC_FARNELL" value="1101541"/>
<attribute name="OC_NEWARK" value="36K7581"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4340" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/sbos073/sbos073.pdf</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA4340UA"/>
<attribute name="OC_FARNELL" value="1212307"/>
<attribute name="OC_NEWARK" value="35C1907"/>
</technology>
</technologies>
</device>
<device name="E" package="SSOP16BU">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="13"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="12"/>
<connect gate="C" pin="-IN" pad="11"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="14"/>
<connect gate="D" pin="-IN" pad="15"/>
<connect gate="D" pin="OUT" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA4340EA/250G4"/>
<attribute name="OC_FARNELL" value="1207061"/>
<attribute name="OC_NEWARK" value="67K8209"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA340" prefix="IC">
<description>&lt;b&gt;Rail-to-Rail Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Single-Supply, MicroAmplifier(TM) Series</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="N" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA340NA/3KG4"/>
<attribute name="OC_FARNELL" value="1234805"/>
<attribute name="OC_NEWARK" value="13M5177"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA340PA"/>
<attribute name="OC_FARNELL" value="1097413"/>
<attribute name="OC_NEWARK" value="97K6826"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA340UA"/>
<attribute name="OC_FARNELL" value="1106196"/>
<attribute name="OC_NEWARK" value="24M5449"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA643" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="2+2-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="+VS1" pad="7"/>
<connect gate="G$1" pin="+VS2" pad="8"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-VS1" pad="4"/>
<connect gate="G$1" pin="-VS2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="+VS1" pad="7"/>
<connect gate="G$1" pin="+VS2" pad="8"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-VS1" pad="4"/>
<connect gate="G$1" pin="-VS2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA643UB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="75C5127"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA643N" prefix="IC">
<description>&lt;b&gt;Wideband Low Distortion, High Gain Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA124U" prefix="IC">
<description>&lt;b&gt;Difet Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SUBS"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="SUBS" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA124U"/>
<attribute name="OC_FARNELL" value="1206923"/>
<attribute name="OC_NEWARK" value="80K6002"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA241" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Single-Supply, MicroPower</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA241PA"/>
<attribute name="OC_FARNELL" value="1097411"/>
<attribute name="OC_NEWARK" value="80K6022"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA241UA"/>
<attribute name="OC_FARNELL" value="1648699"/>
<attribute name="OC_NEWARK" value="75C4749"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA251" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Single-Supply, MicroPower</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA251PA"/>
<attribute name="OC_FARNELL" value="1754989"/>
<attribute name="OC_NEWARK" value="75C4754"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA251UA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="75C4755"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA129" prefix="IC">
<description>&lt;b&gt;Difet Operational Amplifier&lt;/b&gt;&lt;p&gt;
Ultra-Low Bias Current</description>
<gates>
<gate name="G$1" symbol="SUBS"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="SUBS" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="SUBS" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA129U"/>
<attribute name="OC_FARNELL" value="1206925"/>
<attribute name="OC_NEWARK" value="80K6004"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA132" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
High Speed FET-Input</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA132U"/>
<attribute name="OC_FARNELL" value="1823332"/>
<attribute name="OC_NEWARK" value="80K6008"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2132" prefix="IC">
<description>&lt;b&gt;High Speed FET-Input Operational Amplifiers&lt;/b&gt;&lt;
Product Folder:OPA2132</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2132U"/>
<attribute name="OC_FARNELL" value="1206934"/>
<attribute name="OC_NEWARK" value="80K6015"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA2132P"/>
<attribute name="OC_FARNELL" value="1212432"/>
<attribute name="OC_NEWARK" value="47P7461"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4132" prefix="IC">
<description>&lt;b&gt;High Speed FET-Input Operational Amplifiers&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA4132UA"/>
<attribute name="OC_FARNELL" value="1212302"/>
<attribute name="OC_NEWARK" value="80K6028"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA131" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
General Purpose FET-Input</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA131U"/>
<attribute name="OC_FARNELL" value="1459547"/>
<attribute name="OC_NEWARK" value="75C4591"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2131" prefix="IC">
<description>&lt;b&gt;General Purpose FET-Input Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Product Folder:OPA2131</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA2131UJ/2K5"/>
<attribute name="OC_FARNELL" value="1575488"/>
<attribute name="OC_NEWARK" value="75C4620"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4131" prefix="IC">
<description>&lt;b&gt;General Purpose FET-Input Operational Amplifiers&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO16-1">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="13"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="12"/>
<connect gate="C" pin="-IN" pad="11"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="14"/>
<connect gate="D" pin="-IN" pad="15"/>
<connect gate="D" pin="OUT" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA4131UA"/>
<attribute name="OC_FARNELL" value="1459611"/>
<attribute name="OC_NEWARK" value="75C4950"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA4131PA"/>
<attribute name="OC_FARNELL" value="1509638"/>
<attribute name="OC_NEWARK" value="80K6027"/>
</technology>
</technologies>
</device>
<device name="N" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA4131NA"/>
<attribute name="OC_FARNELL" value="1564896"/>
<attribute name="OC_NEWARK" value="80K6025"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA130" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Low Power, Precision FET-Input</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA130UA"/>
<attribute name="OC_FARNELL" value="1577774"/>
<attribute name="OC_NEWARK" value="80K6006"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2130" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="B" symbol="OP-AMP"/>
<gate name="A" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2130UA"/>
<attribute name="OC_FARNELL" value="1459554"/>
<attribute name="OC_NEWARK" value="35C1841"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4130" prefix="IC">
<description>&lt;b&gt;Low Power, Precision FET-Input Operational Amplifiers&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA4130UA"/>
<attribute name="OC_FARNELL" value="1648707"/>
<attribute name="OC_NEWARK" value="80K8080"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA134" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
SoundPlus(TM) High Performance Audio</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA134PA"/>
<attribute name="OC_FARNELL" value="1335032"/>
<attribute name="OC_NEWARK" value="75C4599"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA134UA"/>
<attribute name="OC_FARNELL" value="1097514"/>
<attribute name="OC_NEWARK" value="80K6009"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2134" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2134UA"/>
<attribute name="OC_FARNELL" value="1206935"/>
<attribute name="OC_NEWARK" value="35C1847"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2134PA"/>
<attribute name="OC_FARNELL" value="1097574"/>
<attribute name="OC_NEWARK" value="74K3897"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA177" prefix="IC">
<description>&lt;b&gt;Precision Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA177GPG4"/>
<attribute name="OC_FARNELL" value="1219410"/>
<attribute name="OC_NEWARK" value="05M0933"/>
</technology>
</technologies>
</device>
<device name="S" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA177GS"/>
<attribute name="OC_FARNELL" value="1212431"/>
<attribute name="OC_NEWARK" value="35C0218"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA77" prefix="IC">
<description>&lt;b&gt;Clamping Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA234" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Low Power, Precision, Single-Supply</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA234U"/>
<attribute name="OC_FARNELL" value="1648695"/>
<attribute name="OC_NEWARK" value="75C4693"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2234" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2234U"/>
<attribute name="OC_FARNELL" value="1212441"/>
<attribute name="OC_NEWARK" value="96K4523"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4234" prefix="IC">
<description>&lt;b&gt;Low Power, Precision Single-Supply Operational Amplifiers&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA4234U"/>
<attribute name="OC_FARNELL" value="1207058"/>
<attribute name="OC_NEWARK" value="75C4965"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA237" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Single-Supply, MicroAmplifier(TM) Series</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="N" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA237NA/250"/>
<attribute name="OC_FARNELL" value="4625298"/>
<attribute name="OC_NEWARK" value="35C1874"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA237UA"/>
<attribute name="OC_FARNELL" value="1800507"/>
<attribute name="OC_NEWARK" value="04M4584"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2237" prefix="IC">
<description>&lt;b&gt;Single-Supply Operational Amplifiers&lt;/b&gt;&lt;p&gt;
MicroAmplifier(TM) Series; Product Folder:OPA2237</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="E" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2237EA/250"/>
<attribute name="OC_FARNELL" value="1470365"/>
<attribute name="OC_NEWARK" value="35C1853"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2237UA"/>
<attribute name="OC_FARNELL" value="1388075"/>
<attribute name="OC_NEWARK" value="80K6018"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4237" prefix="IC">
<description>&lt;b&gt;Single-Supply Operational Amplifiers&lt;/b&gt;&lt;p&gt;
MicroAmplifier(TM) Series</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SSOP16BU">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="13"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="12"/>
<connect gate="C" pin="-IN" pad="11"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="14"/>
<connect gate="D" pin="-IN" pad="15"/>
<connect gate="D" pin="OUT" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA336" prefix="IC">
<description>&lt;b&gt;CMOS Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Single-Supply, MicroPower, MicroAmplifier(TM) Series</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="N" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA336NA"/>
<attribute name="OC_FARNELL" value="1212297"/>
<attribute name="OC_NEWARK" value="01M8405"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA336UA"/>
<attribute name="OC_FARNELL" value="1459587"/>
<attribute name="OC_NEWARK" value="35C1888"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2336" prefix="IC">
<description>&lt;b&gt;Single-Supply, MicroPower CMOS Operational Amplifiers&lt;/b&gt;&lt;p&gt;
MicroAmplifier Series; Product Folder:OPA2336,</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="E" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA2336E/250"/>
<attribute name="OC_FARNELL" value="1295989"/>
<attribute name="OC_NEWARK" value="74K3899"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA2336PA."/>
<attribute name="OC_FARNELL" value="1097396"/>
<attribute name="OC_NEWARK" value="26M1908"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA2336UA"/>
<attribute name="OC_FARNELL" value="1106183"/>
<attribute name="OC_NEWARK" value="24M5438"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4336" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Single-Supply, MicroPower CMOS Operational Amplifiers&lt;/b&gt;&lt;p&gt;
MicroAmplifier (TM) Series</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="E" package="SSOP16BU">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="13"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="12"/>
<connect gate="C" pin="-IN" pad="11"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="14"/>
<connect gate="D" pin="-IN" pad="15"/>
<connect gate="D" pin="OUT" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA4336EA/250"/>
<attribute name="OC_FARNELL" value="1207060"/>
<attribute name="OC_NEWARK" value="74K3911"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA627" prefix="IC">
<description>&lt;b&gt;Difet(R) Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Precision, High-Speed</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA627BP"/>
<attribute name="OC_FARNELL" value="1212318"/>
<attribute name="OC_NEWARK" value="35C1918"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA627AU"/>
<attribute name="OC_FARNELL" value="1207067"/>
<attribute name="OC_NEWARK" value="30C4516"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA627M" prefix="IC">
<description>&lt;b&gt;Difet(R) Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Precision, High-Speed</description>
<gates>
<gate name="G$1" symbol="2TRIMCAS"/>
</gates>
<devices>
<device name="" package="TO99">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CASE" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="OPA627AM"/>
<attribute name="OC_FARNELL" value="1459637"/>
<attribute name="OC_NEWARK" value="72K7290"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA637" prefix="IC">
<description>&lt;b&gt;Difet(R) Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Precision, High-Speed</description>
<gates>
<gate name="G$1" symbol="2TRIM"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA637AP."/>
<attribute name="OC_FARNELL" value="1263170"/>
<attribute name="OC_NEWARK" value="75C5108"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA637AU"/>
<attribute name="OC_FARNELL" value="1544014"/>
<attribute name="OC_NEWARK" value="80K6031"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA637M" prefix="IC">
<description>&lt;b&gt;Difet(R) Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Precision, High-Speed</description>
<gates>
<gate name="G$1" symbol="2TRIMCAS"/>
</gates>
<devices>
<device name="" package="TO99">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CASE" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM1" pad="1"/>
<connect gate="G$1" pin="TRIM2" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA637AM"/>
<attribute name="OC_FARNELL" value="1459640"/>
<attribute name="OC_NEWARK" value="61M8069"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA642" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
Wideband, Low Distortion</description>
<gates>
<gate name="G$1" symbol="2+2-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="+VS1" pad="7"/>
<connect gate="G$1" pin="+VS2" pad="8"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-VS1" pad="4"/>
<connect gate="G$1" pin="-VS2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD9631ANZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="19M1012"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA642U" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="2+2-"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="+VS1" pad="7"/>
<connect gate="G$1" pin="+VS2" pad="8"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-VS1" pad="4"/>
<connect gate="G$1" pin="-VS2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD9631ARZ"/>
<attribute name="OC_FARNELL" value="1319480"/>
<attribute name="OC_NEWARK" value="19M8943"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA642N" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
Wideband, Low Distortion</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4658U" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4650" prefix="IC">
<description>&lt;b&gt;Operational Amplifiers&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
<gate name="C" symbol="OP-AMP"/>
<gate name="D" symbol="OP-AMP"/>
</gates>
<devices>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="4"/>
<connect gate="A" pin="V-" pad="11"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2658" prefix="IC">
<description>&lt;b&gt;Dual Wideband, Low Power, Current Feedback Operational Amplifier&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="E" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA658" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
Wideband, Low Power, Current Feedback</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="N" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8001ANZ"/>
<attribute name="OC_FARNELL" value="9605304"/>
<attribute name="OC_NEWARK" value="19M0911"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8001ARZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="19M0912"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2650" prefix="IC">
<description>&lt;b&gt;Dual Wideband, Low Power Voltage Feedback Operational Amplifier&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="A" symbol="OP-AMP+-"/>
<gate name="B" symbol="OP-AMP"/>
</gates>
<devices>
<device name="E" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AD8056ANZ"/>
<attribute name="OC_FARNELL" value="1079308"/>
<attribute name="OC_NEWARK" value="19M0925"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="MPN" value="AD8056ARMZ"/>
<attribute name="OC_FARNELL" value="1424046"/>
<attribute name="OC_NEWARK" value="59K6306"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA678" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
Wideband, Switched-Input</description>
<gates>
<gate name="G$1" symbol="OPA678"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!CHA" pad="12"/>
<connect gate="G$1" pin="+INA" pad="1"/>
<connect gate="G$1" pin="+INB" pad="16"/>
<connect gate="G$1" pin="+VCC" pad="7"/>
<connect gate="G$1" pin="-INA" pad="2"/>
<connect gate="G$1" pin="-INB" pad="15"/>
<connect gate="G$1" pin="-VCC" pad="10"/>
<connect gate="G$1" pin="CCAP" pad="5"/>
<connect gate="G$1" pin="CHA" pad="13"/>
<connect gate="G$1" pin="COM" pad="11"/>
<connect gate="G$1" pin="DNC" pad="14"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="6"/>
<connect gate="G$1" pin="NC@3" pad="9"/>
<connect gate="G$1" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="!CHA" pad="12"/>
<connect gate="G$1" pin="+INA" pad="1"/>
<connect gate="G$1" pin="+INB" pad="16"/>
<connect gate="G$1" pin="+VCC" pad="7"/>
<connect gate="G$1" pin="-INA" pad="2"/>
<connect gate="G$1" pin="-INB" pad="15"/>
<connect gate="G$1" pin="-VCC" pad="10"/>
<connect gate="G$1" pin="CCAP" pad="5"/>
<connect gate="G$1" pin="CHA" pad="13"/>
<connect gate="G$1" pin="COM" pad="11"/>
<connect gate="G$1" pin="DNC" pad="14"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="6"/>
<connect gate="G$1" pin="NC@3" pad="9"/>
<connect gate="G$1" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA655" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
Wideband, FET-Input</description>
<gates>
<gate name="G$1" symbol="2+2-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="+VS1" pad="7"/>
<connect gate="G$1" pin="+VS2" pad="8"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-VS1" pad="4"/>
<connect gate="G$1" pin="-VS2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA655P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="75C5130"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="+VS1" pad="7"/>
<connect gate="G$1" pin="+VS2" pad="8"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-VS1" pad="4"/>
<connect gate="G$1" pin="-VS2" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA650" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
Wideband, Low Power, Voltage Feedback</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="N" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA651" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
Wideband, Low Power, Voltage Feedback</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="N" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1726E" prefix="IC">
<description>&lt;b&gt;Stereo Audio DAC&lt;/b&gt;&lt;p&gt;
16 bit, 96KHz sampling</description>
<gates>
<gate name="G$1" symbol="PCM1726"/>
</gates>
<devices>
<device name="" package="SSOP20BU">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCKIN" pad="14"/>
<connect gate="G$1" pin="CAP" pad="13"/>
<connect gate="G$1" pin="DGND" pad="20"/>
<connect gate="G$1" pin="DIN" pad="15"/>
<connect gate="G$1" pin="FOR" pad="4"/>
<connect gate="G$1" pin="LRCIN" pad="16"/>
<connect gate="G$1" pin="LRPL" pad="5"/>
<connect gate="G$1" pin="MUTE" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="OUTL" pad="12"/>
<connect gate="G$1" pin="OUTR" pad="9"/>
<connect gate="G$1" pin="RES" pad="3"/>
<connect gate="G$1" pin="RES@1" pad="18"/>
<connect gate="G$1" pin="RSTB" pad="7"/>
<connect gate="G$1" pin="SCKI" pad="2"/>
<connect gate="G$1" pin="TEST" pad="17"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VDD" pad="19"/>
<connect gate="G$1" pin="ZERO" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1727E" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio DAC&lt;/b&gt;&lt;p&gt;
with Programmable Dual PLL</description>
<gates>
<gate name="G$1" symbol="PCM1727"/>
</gates>
<devices>
<device name="" package="SSOP24BU">
<connects>
<connect gate="G$1" pin="!RSTB" pad="10"/>
<connect gate="G$1" pin="!ZERO" pad="16"/>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="BCKIN" pad="17"/>
<connect gate="G$1" pin="CAP" pad="15"/>
<connect gate="G$1" pin="DGND" pad="23"/>
<connect gate="G$1" pin="DIN" pad="18"/>
<connect gate="G$1" pin="LRCIN" pad="19"/>
<connect gate="G$1" pin="MC" pad="8"/>
<connect gate="G$1" pin="MCKO" pad="4"/>
<connect gate="G$1" pin="MD" pad="9"/>
<connect gate="G$1" pin="ML" pad="7"/>
<connect gate="G$1" pin="OUTL" pad="14"/>
<connect gate="G$1" pin="OUTR" pad="11"/>
<connect gate="G$1" pin="PGND" pad="2"/>
<connect gate="G$1" pin="RSV" pad="5"/>
<connect gate="G$1" pin="SCKO1" pad="21"/>
<connect gate="G$1" pin="SCKO2" pad="20"/>
<connect gate="G$1" pin="SCKO3" pad="6"/>
<connect gate="G$1" pin="VCA" pad="13"/>
<connect gate="G$1" pin="VCP" pad="3"/>
<connect gate="G$1" pin="VDD" pad="22"/>
<connect gate="G$1" pin="XTI" pad="1"/>
<connect gate="G$1" pin="XTO" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM1727E"/>
<attribute name="OC_FARNELL" value="1408314"/>
<attribute name="OC_NEWARK" value="75C5319"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1725U" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio DAConverter&lt;/b&gt;&lt;p&gt;
16 Bits, 96kHz Sampling</description>
<gates>
<gate name="G$1" symbol="PCM1725"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="BCKIN" pad="3"/>
<connect gate="G$1" pin="CAP" pad="5"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="DM" pad="12"/>
<connect gate="G$1" pin="FOR" pad="13"/>
<connect gate="G$1" pin="LRCIN" pad="1"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NC@1" pad="10"/>
<connect gate="G$1" pin="NC@2" pad="11"/>
<connect gate="G$1" pin="OUTL" pad="9"/>
<connect gate="G$1" pin="OUTR" pad="6"/>
<connect gate="G$1" pin="SCKI" pad="14"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PCM1725U"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="34K8597"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1723E" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio DAC&lt;/b&gt;&lt;p&gt;
with Programmable PLL</description>
<gates>
<gate name="G$1" symbol="PCM1723"/>
</gates>
<devices>
<device name="" package="SSOP24BU">
<connects>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="BCKIN" pad="16"/>
<connect gate="G$1" pin="CAP" pad="15"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="DIN" pad="17"/>
<connect gate="G$1" pin="LRCIN" pad="18"/>
<connect gate="G$1" pin="MC" pad="7"/>
<connect gate="G$1" pin="MCKO" pad="5"/>
<connect gate="G$1" pin="MD" pad="8"/>
<connect gate="G$1" pin="ML" pad="6"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NC@1" pad="19"/>
<connect gate="G$1" pin="OUTL" pad="14"/>
<connect gate="G$1" pin="OUTR" pad="11"/>
<connect gate="G$1" pin="PGND" pad="23"/>
<connect gate="G$1" pin="RES" pad="20"/>
<connect gate="G$1" pin="RSTB" pad="9"/>
<connect gate="G$1" pin="SCKO" pad="2"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VCP" pad="3"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="XTI" pad="1"/>
<connect gate="G$1" pin="XTO" pad="24"/>
<connect gate="G$1" pin="ZERO" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCM1723EG4"/>
<attribute name="OC_FARNELL" value="1234896"/>
<attribute name="OC_NEWARK" value="66K4046"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1717E" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM1717"/>
</gates>
<devices>
<device name="" package="SSOP20BU">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCKIN" pad="6"/>
<connect gate="G$1" pin="CLKO" pad="19"/>
<connect gate="G$1" pin="D/C_L" pad="13"/>
<connect gate="G$1" pin="D/C_R" pad="8"/>
<connect gate="G$1" pin="DGND" pad="2"/>
<connect gate="G$1" pin="DIN" pad="5"/>
<connect gate="G$1" pin="LRCIN" pad="4"/>
<connect gate="G$1" pin="MC/DM1" pad="17"/>
<connect gate="G$1" pin="MD/DM0" pad="16"/>
<connect gate="G$1" pin="ML/MUTE" pad="18"/>
<connect gate="G$1" pin="MODE" pad="14"/>
<connect gate="G$1" pin="OUTL" pad="12"/>
<connect gate="G$1" pin="OUTR" pad="9"/>
<connect gate="G$1" pin="RSTB" pad="15"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="XTI" pad="1"/>
<connect gate="G$1" pin="XTO" pad="20"/>
<connect gate="G$1" pin="ZERO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PCM1717E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="34K8595"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1715U" prefix="IC">
<description>&lt;b&gt;Dual Voltage Output CMOS Delta-Sigma DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM1715"/>
</gates>
<devices>
<device name="" package="SOJ28-4">
<connects>
<connect gate="G$1" pin="AGND1" pad="14"/>
<connect gate="G$1" pin="AGND2L" pad="19"/>
<connect gate="G$1" pin="AGND2R" pad="10"/>
<connect gate="G$1" pin="BCKIN" pad="3"/>
<connect gate="G$1" pin="CKSL" pad="23"/>
<connect gate="G$1" pin="CLKO" pad="4"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="EXT1L" pad="18"/>
<connect gate="G$1" pin="EXT1R" pad="11"/>
<connect gate="G$1" pin="EXT2L" pad="17"/>
<connect gate="G$1" pin="EXT2R" pad="12"/>
<connect gate="G$1" pin="LRCIN" pad="1"/>
<connect gate="G$1" pin="MC" pad="27"/>
<connect gate="G$1" pin="MD" pad="26"/>
<connect gate="G$1" pin="ML" pad="28"/>
<connect gate="G$1" pin="NC" pad="24"/>
<connect gate="G$1" pin="OUTL" pad="16"/>
<connect gate="G$1" pin="OUTR" pad="13"/>
<connect gate="G$1" pin="RSTB" pad="25"/>
<connect gate="G$1" pin="VCC1" pad="15"/>
<connect gate="G$1" pin="VCC2L" pad="20"/>
<connect gate="G$1" pin="VCC2R" pad="9"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VDD@1" pad="21"/>
<connect gate="G$1" pin="XTI" pad="5"/>
<connect gate="G$1" pin="XTO" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1721E" prefix="IC">
<description>&lt;b&gt;SoundPlus Stereo Audio DAC&lt;/b&gt;&lt;p&gt;
MPEG2/AC-3 Compatible</description>
<gates>
<gate name="G$1" symbol="PCM1721"/>
</gates>
<devices>
<device name="" package="SSOP24BU">
<connects>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="BCKIN" pad="16"/>
<connect gate="G$1" pin="CAP" pad="15"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="DIN" pad="17"/>
<connect gate="G$1" pin="LRCIN" pad="18"/>
<connect gate="G$1" pin="MC" pad="7"/>
<connect gate="G$1" pin="MCKI" pad="1"/>
<connect gate="G$1" pin="MD" pad="8"/>
<connect gate="G$1" pin="ML" pad="6"/>
<connect gate="G$1" pin="NC" pad="24"/>
<connect gate="G$1" pin="OUTL" pad="14"/>
<connect gate="G$1" pin="OUTR" pad="11"/>
<connect gate="G$1" pin="PGND" pad="23"/>
<connect gate="G$1" pin="RES" pad="5"/>
<connect gate="G$1" pin="RES@1" pad="20"/>
<connect gate="G$1" pin="RSTB" pad="9"/>
<connect gate="G$1" pin="SCKI" pad="4"/>
<connect gate="G$1" pin="SCKO" pad="2"/>
<connect gate="G$1" pin="TEST" pad="19"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VCP" pad="3"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="ZERO" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1720E" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio DAC&lt;/b&gt;&lt;p&gt;
MPEG2/AC-3 Compatible</description>
<gates>
<gate name="G$1" symbol="PCM1720"/>
</gates>
<devices>
<device name="" package="SSOP20BU">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCKIN" pad="14"/>
<connect gate="G$1" pin="CAP" pad="13"/>
<connect gate="G$1" pin="DGND" pad="20"/>
<connect gate="G$1" pin="DIN" pad="15"/>
<connect gate="G$1" pin="LRCIN" pad="16"/>
<connect gate="G$1" pin="MC" pad="5"/>
<connect gate="G$1" pin="MD" pad="6"/>
<connect gate="G$1" pin="ML" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="17"/>
<connect gate="G$1" pin="NC@2" pad="18"/>
<connect gate="G$1" pin="OUTL" pad="12"/>
<connect gate="G$1" pin="OUTR" pad="9"/>
<connect gate="G$1" pin="RSTB" pad="7"/>
<connect gate="G$1" pin="SCKI" pad="2"/>
<connect gate="G$1" pin="TEST" pad="3"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VDD" pad="19"/>
<connect gate="G$1" pin="ZERO" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCM1720E/2KG4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="66K4045"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1719E" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM1719"/>
</gates>
<devices>
<device name="" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCKIN" pad="6"/>
<connect gate="G$1" pin="CLKO" pad="27"/>
<connect gate="G$1" pin="COM" pad="21"/>
<connect gate="G$1" pin="DGND" pad="2"/>
<connect gate="G$1" pin="DIN" pad="5"/>
<connect gate="G$1" pin="LRCIN" pad="4"/>
<connect gate="G$1" pin="MC" pad="25"/>
<connect gate="G$1" pin="MD" pad="24"/>
<connect gate="G$1" pin="ML" pad="26"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="22"/>
<connect gate="G$1" pin="OUTL" pad="20"/>
<connect gate="G$1" pin="OUTR" pad="9"/>
<connect gate="G$1" pin="PAGND" pad="14"/>
<connect gate="G$1" pin="PCOM" pad="12"/>
<connect gate="G$1" pin="PINL" pad="18"/>
<connect gate="G$1" pin="PINR" pad="11"/>
<connect gate="G$1" pin="PMUTE" pad="17"/>
<connect gate="G$1" pin="POUTL" pad="16"/>
<connect gate="G$1" pin="POUTR" pad="13"/>
<connect gate="G$1" pin="PVCC" pad="15"/>
<connect gate="G$1" pin="RSTB" pad="23"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="XTI" pad="1"/>
<connect gate="G$1" pin="XTO" pad="28"/>
<connect gate="G$1" pin="ZERO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCM1719E/2KG4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="67K8259"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1718E" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM1718"/>
</gates>
<devices>
<device name="" package="SSOP20DB">
<connects>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCKIN" pad="6"/>
<connect gate="G$1" pin="CLKO" pad="19"/>
<connect gate="G$1" pin="D/C_L" pad="13"/>
<connect gate="G$1" pin="D/C_R" pad="8"/>
<connect gate="G$1" pin="DGND" pad="2"/>
<connect gate="G$1" pin="DIN" pad="5"/>
<connect gate="G$1" pin="DM0" pad="16"/>
<connect gate="G$1" pin="DM1" pad="17"/>
<connect gate="G$1" pin="FOR" pad="14"/>
<connect gate="G$1" pin="LRCIN" pad="4"/>
<connect gate="G$1" pin="MUTE" pad="18"/>
<connect gate="G$1" pin="OUTL" pad="12"/>
<connect gate="G$1" pin="OUTR" pad="9"/>
<connect gate="G$1" pin="RSTB" pad="15"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VDD" pad="3"/>
<connect gate="G$1" pin="XTI" pad="1"/>
<connect gate="G$1" pin="XTO" pad="20"/>
<connect gate="G$1" pin="ZERO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM1718E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="35C1942"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1702P" prefix="IC">
<description>&lt;b&gt;BiCMOS Advanced Sign Magnitude 20-Bit DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM1702"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="+VCC" pad="9"/>
<connect gate="G$1" pin="+VDD" pad="3"/>
<connect gate="G$1" pin="-VCC" pad="16"/>
<connect gate="G$1" pin="-VDD" pad="5"/>
<connect gate="G$1" pin="ACOM" pad="12"/>
<connect gate="G$1" pin="ACOM@1" pad="13"/>
<connect gate="G$1" pin="BPO" pad="10"/>
<connect gate="G$1" pin="CLOCK" pad="2"/>
<connect gate="G$1" pin="DATA" pad="1"/>
<connect gate="G$1" pin="DCOM" pad="4"/>
<connect gate="G$1" pin="IOUT" pad="11"/>
<connect gate="G$1" pin="LE" pad="6"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="NC@1" pad="8"/>
<connect gate="G$1" pin="REF" pad="15"/>
<connect gate="G$1" pin="SERV" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM1702P-J"/>
<attribute name="OC_FARNELL" value="1509912"/>
<attribute name="OC_NEWARK" value="75C5298"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1702U" prefix="IC">
<description>&lt;b&gt;BiCMOS Advanced Sign Magnitude 20-Bit DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM1702U"/>
</gates>
<devices>
<device name="" package="SO20L">
<connects>
<connect gate="G$1" pin="+VCC" pad="11"/>
<connect gate="G$1" pin="+VDD" pad="4"/>
<connect gate="G$1" pin="-VCC" pad="20"/>
<connect gate="G$1" pin="-VDD" pad="6"/>
<connect gate="G$1" pin="ACOM" pad="15"/>
<connect gate="G$1" pin="ACOM@1" pad="16"/>
<connect gate="G$1" pin="BPO" pad="12"/>
<connect gate="G$1" pin="CLOCK" pad="2"/>
<connect gate="G$1" pin="DATA" pad="1"/>
<connect gate="G$1" pin="DCOM" pad="5"/>
<connect gate="G$1" pin="IOUT" pad="14"/>
<connect gate="G$1" pin="LE" pad="7"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="8"/>
<connect gate="G$1" pin="NC@2" pad="9"/>
<connect gate="G$1" pin="NC@3" pad="10"/>
<connect gate="G$1" pin="NC@4" pad="13"/>
<connect gate="G$1" pin="NC@5" pad="18"/>
<connect gate="G$1" pin="REF" pad="19"/>
<connect gate="G$1" pin="SERV" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM1702U"/>
<attribute name="OC_FARNELL" value="1509914"/>
<attribute name="OC_NEWARK" value="75C5299"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1710U" prefix="IC">
<description>&lt;b&gt;Dual Voltage Output CMOS Delta-Sigma DAC&lt;/b&gt;&lt;p&gt;
with On-Chip Digital Filter</description>
<gates>
<gate name="G$1" symbol="PCM1710"/>
</gates>
<devices>
<device name="" package="SO28-3">
<connects>
<connect gate="G$1" pin="AGND1" pad="14"/>
<connect gate="G$1" pin="AGND2L" pad="19"/>
<connect gate="G$1" pin="AGND2R" pad="10"/>
<connect gate="G$1" pin="BCKIN" pad="3"/>
<connect gate="G$1" pin="CKSL" pad="23"/>
<connect gate="G$1" pin="CLKO" pad="4"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="EXT1L" pad="18"/>
<connect gate="G$1" pin="EXT1R" pad="11"/>
<connect gate="G$1" pin="EXT2L" pad="17"/>
<connect gate="G$1" pin="EXT2R" pad="12"/>
<connect gate="G$1" pin="LRCIN" pad="1"/>
<connect gate="G$1" pin="MC/DM1" pad="26"/>
<connect gate="G$1" pin="MC/DM2" pad="27"/>
<connect gate="G$1" pin="ML/DSD" pad="28"/>
<connect gate="G$1" pin="MODE" pad="24"/>
<connect gate="G$1" pin="MUTE" pad="25"/>
<connect gate="G$1" pin="OUTL" pad="16"/>
<connect gate="G$1" pin="OUTR" pad="13"/>
<connect gate="G$1" pin="VCC1" pad="15"/>
<connect gate="G$1" pin="VCC2L" pad="20"/>
<connect gate="G$1" pin="VCC2R" pad="9"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VDD@1" pad="21"/>
<connect gate="G$1" pin="XTI" pad="5"/>
<connect gate="G$1" pin="XTO" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM1710U"/>
<attribute name="OC_FARNELL" value="1212857"/>
<attribute name="OC_NEWARK" value="75C5309"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1800E" prefix="IC">
<description>&lt;b&gt;Single-Ended Analog Input 20-Bit Stereo ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM1800"/>
</gates>
<devices>
<device name="" package="SSOP24BU">
<connects>
<connect gate="G$1" pin="AGND" pad="24"/>
<connect gate="G$1" pin="BCK" pad="14"/>
<connect gate="G$1" pin="BYPAS" pad="7"/>
<connect gate="G$1" pin="CNL" pad="21"/>
<connect gate="G$1" pin="CNR" pad="19"/>
<connect gate="G$1" pin="CPL" pad="22"/>
<connect gate="G$1" pin="CPR" pad="20"/>
<connect gate="G$1" pin="DGND" pad="17"/>
<connect gate="G$1" pin="FMT0" pad="8"/>
<connect gate="G$1" pin="FMT1" pad="9"/>
<connect gate="G$1" pin="FSYNC" pad="12"/>
<connect gate="G$1" pin="INL" pad="1"/>
<connect gate="G$1" pin="INR" pad="5"/>
<connect gate="G$1" pin="LRCK" pad="13"/>
<connect gate="G$1" pin="MODE0" pad="10"/>
<connect gate="G$1" pin="MODE1" pad="11"/>
<connect gate="G$1" pin="OUT" pad="15"/>
<connect gate="G$1" pin="REF1" pad="2"/>
<connect gate="G$1" pin="REF2" pad="4"/>
<connect gate="G$1" pin="REFCOM" pad="3"/>
<connect gate="G$1" pin="RSTB" pad="6"/>
<connect gate="G$1" pin="SYSCLK" pad="16"/>
<connect gate="G$1" pin="VCC" pad="23"/>
<connect gate="G$1" pin="VDD" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PCM1800E"/>
<attribute name="OC_FARNELL" value="1648631"/>
<attribute name="OC_NEWARK" value="34K8598"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM3000E" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio Codec&lt;/b&gt;&lt;p&gt;
18-bits, Serial Interface</description>
<gates>
<gate name="G$1" symbol="PCM3000"/>
</gates>
<devices>
<device name="" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="AGND1" pad="3"/>
<connect gate="G$1" pin="AGND2" pad="13"/>
<connect gate="G$1" pin="BCKIN" pad="17"/>
<connect gate="G$1" pin="CLKIO" pad="22"/>
<connect gate="G$1" pin="CNL" pad="9"/>
<connect gate="G$1" pin="CNR" pad="8"/>
<connect gate="G$1" pin="CPL" pad="10"/>
<connect gate="G$1" pin="CPR" pad="7"/>
<connect gate="G$1" pin="DGND" pad="24"/>
<connect gate="G$1" pin="DIN" pad="18"/>
<connect gate="G$1" pin="DOUT" pad="19"/>
<connect gate="G$1" pin="INL" pad="1"/>
<connect gate="G$1" pin="INR" pad="6"/>
<connect gate="G$1" pin="LRCIN" pad="16"/>
<connect gate="G$1" pin="MC" pad="25"/>
<connect gate="G$1" pin="MD" pad="26"/>
<connect gate="G$1" pin="ML" pad="27"/>
<connect gate="G$1" pin="OUTL" pad="15"/>
<connect gate="G$1" pin="OUTR" pad="12"/>
<connect gate="G$1" pin="REFL" pad="4"/>
<connect gate="G$1" pin="REFR" pad="5"/>
<connect gate="G$1" pin="RSTB" pad="28"/>
<connect gate="G$1" pin="VCC1" pad="2"/>
<connect gate="G$1" pin="VCC2" pad="14"/>
<connect gate="G$1" pin="VCOM" pad="11"/>
<connect gate="G$1" pin="VDD" pad="23"/>
<connect gate="G$1" pin="XTIN" pad="20"/>
<connect gate="G$1" pin="XTO" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCM3000E/2KG4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="67K8276"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM3001E" prefix="IC">
<description>&lt;b&gt;SoundPlus(TM) Stereo Audio Codec&lt;/b&gt;&lt;p&gt;
18-bits, Serial Interface</description>
<gates>
<gate name="G$1" symbol="PCM3001"/>
</gates>
<devices>
<device name="" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="AGND1" pad="3"/>
<connect gate="G$1" pin="AGND2" pad="13"/>
<connect gate="G$1" pin="BCKIN" pad="17"/>
<connect gate="G$1" pin="CLKIO" pad="22"/>
<connect gate="G$1" pin="CNL" pad="9"/>
<connect gate="G$1" pin="CNR" pad="8"/>
<connect gate="G$1" pin="CPL" pad="10"/>
<connect gate="G$1" pin="CPR" pad="7"/>
<connect gate="G$1" pin="DGND" pad="24"/>
<connect gate="G$1" pin="DIN" pad="18"/>
<connect gate="G$1" pin="DOUT" pad="19"/>
<connect gate="G$1" pin="FMT0" pad="27"/>
<connect gate="G$1" pin="FMT1" pad="26"/>
<connect gate="G$1" pin="FMT2" pad="25"/>
<connect gate="G$1" pin="INL" pad="1"/>
<connect gate="G$1" pin="INR" pad="6"/>
<connect gate="G$1" pin="LRCIN" pad="16"/>
<connect gate="G$1" pin="OUTL" pad="15"/>
<connect gate="G$1" pin="OUTR" pad="12"/>
<connect gate="G$1" pin="REFL" pad="4"/>
<connect gate="G$1" pin="REFR" pad="5"/>
<connect gate="G$1" pin="RSTB" pad="28"/>
<connect gate="G$1" pin="VCC1" pad="2"/>
<connect gate="G$1" pin="VCC2" pad="14"/>
<connect gate="G$1" pin="VCOM" pad="11"/>
<connect gate="G$1" pin="VDD" pad="23"/>
<connect gate="G$1" pin="XTIN" pad="20"/>
<connect gate="G$1" pin="XTO" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PCM3001E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="34K8600"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1712U" prefix="IC">
<description>&lt;b&gt;Dual Voltage Output CMOS Delta-Sigma DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM1712"/>
</gates>
<devices>
<device name="" package="SO28-3">
<connects>
<connect gate="G$1" pin="AGND1" pad="14"/>
<connect gate="G$1" pin="AGND2L" pad="19"/>
<connect gate="G$1" pin="AGND2R" pad="10"/>
<connect gate="G$1" pin="BCKIN" pad="3"/>
<connect gate="G$1" pin="CLKO" pad="4"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="DIN" pad="2"/>
<connect gate="G$1" pin="EXT1L" pad="18"/>
<connect gate="G$1" pin="EXT1R" pad="11"/>
<connect gate="G$1" pin="EXT2L" pad="17"/>
<connect gate="G$1" pin="EXT2R" pad="12"/>
<connect gate="G$1" pin="LRCIN" pad="1"/>
<connect gate="G$1" pin="MC/DM1" pad="26"/>
<connect gate="G$1" pin="MC/DM2" pad="27"/>
<connect gate="G$1" pin="ML/DSD" pad="28"/>
<connect gate="G$1" pin="MODE" pad="24"/>
<connect gate="G$1" pin="MUTE" pad="25"/>
<connect gate="G$1" pin="NC" pad="23"/>
<connect gate="G$1" pin="OUTL" pad="16"/>
<connect gate="G$1" pin="OUTR" pad="13"/>
<connect gate="G$1" pin="VCC1" pad="15"/>
<connect gate="G$1" pin="VCC2L" pad="20"/>
<connect gate="G$1" pin="VCC2R" pad="9"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VDD@1" pad="21"/>
<connect gate="G$1" pin="XTI" pad="5"/>
<connect gate="G$1" pin="XTO" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PGA206" prefix="IC">
<description>&lt;b&gt;High-Speed Programmable Gain Instrumentation Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PGA206"/>
</gates>
<devices>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="10"/>
<connect gate="G$1" pin="SENSE" pad="12"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VO1" pad="1"/>
<connect gate="G$1" pin="VO2" pad="9"/>
<connect gate="G$1" pin="VOS" pad="6"/>
<connect gate="G$1" pin="VOS@1" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PGA206UA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="35C1960"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="10"/>
<connect gate="G$1" pin="SENSE" pad="12"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VO1" pad="1"/>
<connect gate="G$1" pin="VO2" pad="9"/>
<connect gate="G$1" pin="VOS" pad="6"/>
<connect gate="G$1" pin="VOS@1" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PGA206PA"/>
<attribute name="OC_FARNELL" value="1470400"/>
<attribute name="OC_NEWARK" value="75C5426"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PGA207" prefix="IC">
<description>&lt;b&gt;High-Speed Programmable Gain Instrumentation Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PGA206"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="10"/>
<connect gate="G$1" pin="SENSE" pad="12"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VO1" pad="1"/>
<connect gate="G$1" pin="VO2" pad="9"/>
<connect gate="G$1" pin="VOS" pad="6"/>
<connect gate="G$1" pin="VOS@1" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="10"/>
<connect gate="G$1" pin="SENSE" pad="12"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="8"/>
<connect gate="G$1" pin="VO1" pad="1"/>
<connect gate="G$1" pin="VO2" pad="9"/>
<connect gate="G$1" pin="VOS" pad="6"/>
<connect gate="G$1" pin="VOS@1" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PGA207UA"/>
<attribute name="OC_FARNELL" value="1212338"/>
<attribute name="OC_NEWARK" value="75C5427"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF102" prefix="IC">
<description>&lt;b&gt;10.0V Precision Voltage Reference&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="REF102"/>
</gates>
<devices>
<device name="M" package="TO99">
<connects>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="7"/>
<connect gate="G$1" pin="NR" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="7"/>
<connect gate="G$1" pin="NR" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="REF102AP"/>
<attribute name="OC_FARNELL" value="1097429"/>
<attribute name="OC_NEWARK" value="10M5244"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="7"/>
<connect gate="G$1" pin="NR" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="TRIM" pad="5"/>
<connect gate="G$1" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="REF102AU"/>
<attribute name="OC_FARNELL" value="1212344"/>
<attribute name="OC_NEWARK" value="04M4600"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF200" prefix="IC">
<description>&lt;b&gt;Dual Current Source/Current Sink&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="REF200"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="I1H" pad="8"/>
<connect gate="G$1" pin="I1L" pad="1"/>
<connect gate="G$1" pin="I2H" pad="7"/>
<connect gate="G$1" pin="I2L" pad="2"/>
<connect gate="G$1" pin="MCOM" pad="3"/>
<connect gate="G$1" pin="MIN" pad="5"/>
<connect gate="G$1" pin="MOUT" pad="4"/>
<connect gate="G$1" pin="SUBST" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="I1H" pad="8"/>
<connect gate="G$1" pin="I1L" pad="1"/>
<connect gate="G$1" pin="I2H" pad="7"/>
<connect gate="G$1" pin="I2L" pad="2"/>
<connect gate="G$1" pin="MCOM" pad="3"/>
<connect gate="G$1" pin="MIN" pad="5"/>
<connect gate="G$1" pin="MOUT" pad="4"/>
<connect gate="G$1" pin="SUBST" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="REF200AU"/>
<attribute name="OC_FARNELL" value="1207240"/>
<attribute name="OC_NEWARK" value="34C7615"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF1004" prefix="IC">
<description>&lt;b&gt;Micropower Voltage Reference&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="REF1004"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="4"/>
<connect gate="G$1" pin="C" pad="6"/>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@2" pad="3"/>
<connect gate="G$1" pin="NC@3" pad="5"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="REF1004C-1.2"/>
<attribute name="OC_FARNELL" value="1296022"/>
<attribute name="OC_NEWARK" value="75C7399"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTR101P" prefix="IC">
<description>&lt;b&gt;BURR-BROWN&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="XTR101"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+IN" pad="4"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="BCONT" pad="12"/>
<connect gate="G$1" pin="BW" pad="13"/>
<connect gate="G$1" pin="E" pad="9"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="REF1" pad="10"/>
<connect gate="G$1" pin="REF2" pad="11"/>
<connect gate="G$1" pin="SPAN" pad="5"/>
<connect gate="G$1" pin="SPAN@1" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="ZA" pad="1"/>
<connect gate="G$1" pin="ZA@1" pad="2"/>
<connect gate="G$1" pin="ZA@2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="XTR101AP"/>
<attribute name="OC_FARNELL" value="1648756"/>
<attribute name="OC_NEWARK" value="84K4518"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTR101U" prefix="IC">
<description>&lt;b&gt;4-20mA Current loop Transmitter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="XTR101U"/>
</gates>
<devices>
<device name="" package="SO16-1">
<connects>
<connect gate="G$1" pin="+IN" pad="4"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="BCONT" pad="14"/>
<connect gate="G$1" pin="BW" pad="15"/>
<connect gate="G$1" pin="E" pad="11"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="9"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="REF1" pad="12"/>
<connect gate="G$1" pin="REF2" pad="13"/>
<connect gate="G$1" pin="SPAN" pad="5"/>
<connect gate="G$1" pin="SPAN@1" pad="6"/>
<connect gate="G$1" pin="VCC" pad="10"/>
<connect gate="G$1" pin="ZA" pad="1"/>
<connect gate="G$1" pin="ZA@1" pad="2"/>
<connect gate="G$1" pin="ZA@2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="XTR101AU"/>
<attribute name="OC_FARNELL" value="6543315"/>
<attribute name="OC_NEWARK" value="77C3626"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC712" prefix="IC">
<description>&lt;b&gt;16-Bit DAC with 16-Bit Bus Interface&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DAC712"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!CLR" pad="9"/>
<connect gate="G$1" pin="!WR" pad="10"/>
<connect gate="G$1" pin="+VCC" pad="7"/>
<connect gate="G$1" pin="-VCC" pad="8"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="ACOM" pad="2"/>
<connect gate="G$1" pin="D0" pad="28"/>
<connect gate="G$1" pin="D1" pad="27"/>
<connect gate="G$1" pin="D10" pad="18"/>
<connect gate="G$1" pin="D11" pad="17"/>
<connect gate="G$1" pin="D12" pad="16"/>
<connect gate="G$1" pin="D13" pad="15"/>
<connect gate="G$1" pin="D14" pad="14"/>
<connect gate="G$1" pin="D15" pad="13"/>
<connect gate="G$1" pin="D2" pad="26"/>
<connect gate="G$1" pin="D3" pad="25"/>
<connect gate="G$1" pin="D4" pad="24"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="22"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="D8" pad="20"/>
<connect gate="G$1" pin="D9" pad="19"/>
<connect gate="G$1" pin="DCOM" pad="1"/>
<connect gate="G$1" pin="GA" pad="6"/>
<connect gate="G$1" pin="OA" pad="4"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="REF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DAC712U"/>
<attribute name="OC_FARNELL" value="1097510"/>
<attribute name="OC_NEWARK" value="74C9132"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!CLR" pad="9"/>
<connect gate="G$1" pin="!WR" pad="10"/>
<connect gate="G$1" pin="+VCC" pad="7"/>
<connect gate="G$1" pin="-VCC" pad="8"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="ACOM" pad="2"/>
<connect gate="G$1" pin="D0" pad="28"/>
<connect gate="G$1" pin="D1" pad="27"/>
<connect gate="G$1" pin="D10" pad="18"/>
<connect gate="G$1" pin="D11" pad="17"/>
<connect gate="G$1" pin="D12" pad="16"/>
<connect gate="G$1" pin="D13" pad="15"/>
<connect gate="G$1" pin="D14" pad="14"/>
<connect gate="G$1" pin="D15" pad="13"/>
<connect gate="G$1" pin="D2" pad="26"/>
<connect gate="G$1" pin="D3" pad="25"/>
<connect gate="G$1" pin="D4" pad="24"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="22"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="D8" pad="20"/>
<connect gate="G$1" pin="D9" pad="19"/>
<connect gate="G$1" pin="DCOM" pad="1"/>
<connect gate="G$1" pin="GA" pad="6"/>
<connect gate="G$1" pin="OA" pad="4"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="REF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="DAC712P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="04M4506"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC714" prefix="IC">
<description>&lt;b&gt;16-Bit DAC with Serial Data Interface&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DAC714"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!CLK" pad="1"/>
<connect gate="G$1" pin="!CLR" pad="16"/>
<connect gate="G$1" pin="+VCC" pad="7"/>
<connect gate="G$1" pin="-VCC" pad="15"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="ACOM" pad="8"/>
<connect gate="G$1" pin="BPO" pad="11"/>
<connect gate="G$1" pin="DCOM" pad="6"/>
<connect gate="G$1" pin="FB2" pad="10"/>
<connect gate="G$1" pin="GA" pad="14"/>
<connect gate="G$1" pin="OA" pad="13"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="REF" pad="12"/>
<connect gate="G$1" pin="SDI" pad="4"/>
<connect gate="G$1" pin="SDO" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="DAC714P"/>
<attribute name="OC_FARNELL" value="1254318"/>
<attribute name="OC_NEWARK" value="78K7952"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="!CLK" pad="1"/>
<connect gate="G$1" pin="!CLR" pad="16"/>
<connect gate="G$1" pin="+VCC" pad="7"/>
<connect gate="G$1" pin="-VCC" pad="15"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="ACOM" pad="8"/>
<connect gate="G$1" pin="BPO" pad="11"/>
<connect gate="G$1" pin="DCOM" pad="6"/>
<connect gate="G$1" pin="FB2" pad="10"/>
<connect gate="G$1" pin="GA" pad="14"/>
<connect gate="G$1" pin="OA" pad="13"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="REF" pad="12"/>
<connect gate="G$1" pin="SDI" pad="4"/>
<connect gate="G$1" pin="SDO" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DAC714U"/>
<attribute name="OC_FARNELL" value="1214385"/>
<attribute name="OC_NEWARK" value="17M6575"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC715" prefix="IC">
<description>&lt;b&gt;16-Bit DAC with 16-Bit Bus Interface&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DAC712"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!CLR" pad="9"/>
<connect gate="G$1" pin="!WR" pad="10"/>
<connect gate="G$1" pin="+VCC" pad="7"/>
<connect gate="G$1" pin="-VCC" pad="8"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="ACOM" pad="2"/>
<connect gate="G$1" pin="D0" pad="28"/>
<connect gate="G$1" pin="D1" pad="27"/>
<connect gate="G$1" pin="D10" pad="18"/>
<connect gate="G$1" pin="D11" pad="17"/>
<connect gate="G$1" pin="D12" pad="16"/>
<connect gate="G$1" pin="D13" pad="15"/>
<connect gate="G$1" pin="D14" pad="14"/>
<connect gate="G$1" pin="D15" pad="13"/>
<connect gate="G$1" pin="D2" pad="26"/>
<connect gate="G$1" pin="D3" pad="25"/>
<connect gate="G$1" pin="D4" pad="24"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="22"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="D8" pad="20"/>
<connect gate="G$1" pin="D9" pad="19"/>
<connect gate="G$1" pin="DCOM" pad="1"/>
<connect gate="G$1" pin="GA" pad="6"/>
<connect gate="G$1" pin="OA" pad="4"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="REF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="DAC715U"/>
<attribute name="OC_FARNELL" value="1509882"/>
<attribute name="OC_NEWARK" value="74C9141"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!CLR" pad="9"/>
<connect gate="G$1" pin="!WR" pad="10"/>
<connect gate="G$1" pin="+VCC" pad="7"/>
<connect gate="G$1" pin="-VCC" pad="8"/>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="11"/>
<connect gate="G$1" pin="ACOM" pad="2"/>
<connect gate="G$1" pin="D0" pad="28"/>
<connect gate="G$1" pin="D1" pad="27"/>
<connect gate="G$1" pin="D10" pad="18"/>
<connect gate="G$1" pin="D11" pad="17"/>
<connect gate="G$1" pin="D12" pad="16"/>
<connect gate="G$1" pin="D13" pad="15"/>
<connect gate="G$1" pin="D14" pad="14"/>
<connect gate="G$1" pin="D15" pad="13"/>
<connect gate="G$1" pin="D2" pad="26"/>
<connect gate="G$1" pin="D3" pad="25"/>
<connect gate="G$1" pin="D4" pad="24"/>
<connect gate="G$1" pin="D5" pad="23"/>
<connect gate="G$1" pin="D6" pad="22"/>
<connect gate="G$1" pin="D7" pad="21"/>
<connect gate="G$1" pin="D8" pad="20"/>
<connect gate="G$1" pin="D9" pad="19"/>
<connect gate="G$1" pin="DCOM" pad="1"/>
<connect gate="G$1" pin="GA" pad="6"/>
<connect gate="G$1" pin="OA" pad="4"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="REF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DAC715P"/>
<attribute name="OC_FARNELL" value="1460194"/>
<attribute name="OC_NEWARK" value="61M5731"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC725" prefix="IC">
<description>&lt;b&gt;Dual 16-Bit DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DAC725"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!A0" pad="4"/>
<connect gate="G$1" pin="!A1" pad="5"/>
<connect gate="G$1" pin="!A2" pad="3"/>
<connect gate="G$1" pin="!CLR" pad="1"/>
<connect gate="G$1" pin="!CSA" pad="23"/>
<connect gate="G$1" pin="!CSB" pad="20"/>
<connect gate="G$1" pin="!WRA" pad="24"/>
<connect gate="G$1" pin="!WRB" pad="19"/>
<connect gate="G$1" pin="+VCC" pad="21"/>
<connect gate="G$1" pin="-VCC" pad="22"/>
<connect gate="G$1" pin="ACOMA" pad="26"/>
<connect gate="G$1" pin="ACOMB" pad="16"/>
<connect gate="G$1" pin="D0" pad="13"/>
<connect gate="G$1" pin="D1" pad="12"/>
<connect gate="G$1" pin="D2" pad="11"/>
<connect gate="G$1" pin="D3" pad="10"/>
<connect gate="G$1" pin="D4" pad="9"/>
<connect gate="G$1" pin="D5" pad="8"/>
<connect gate="G$1" pin="D6" pad="7"/>
<connect gate="G$1" pin="D7" pad="6"/>
<connect gate="G$1" pin="DCOM" pad="14"/>
<connect gate="G$1" pin="GAA" pad="28"/>
<connect gate="G$1" pin="GAB" pad="18"/>
<connect gate="G$1" pin="OUTA" pad="25"/>
<connect gate="G$1" pin="OUTB" pad="15"/>
<connect gate="G$1" pin="SJA" pad="27"/>
<connect gate="G$1" pin="SJB" pad="17"/>
<connect gate="G$1" pin="VDD" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="DAC725JP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="35C0448"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC813" prefix="IC">
<description>&lt;b&gt;Microprocessor-Compatible 12-Bit DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DAC813"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!LDAC" pad="12"/>
<connect gate="G$1" pin="!LLSB" pad="15"/>
<connect gate="G$1" pin="!LMSB" pad="14"/>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="!WR" pad="11"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="+VL" pad="1"/>
<connect gate="G$1" pin="-VCC" pad="10"/>
<connect gate="G$1" pin="ACOM" pad="5"/>
<connect gate="G$1" pin="BPO" pad="4"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="18"/>
<connect gate="G$1" pin="D10" pad="27"/>
<connect gate="G$1" pin="D11" pad="28"/>
<connect gate="G$1" pin="D2" pad="19"/>
<connect gate="G$1" pin="D3" pad="20"/>
<connect gate="G$1" pin="D4" pad="21"/>
<connect gate="G$1" pin="D5" pad="22"/>
<connect gate="G$1" pin="D6" pad="23"/>
<connect gate="G$1" pin="D7" pad="24"/>
<connect gate="G$1" pin="D8" pad="25"/>
<connect gate="G$1" pin="D9" pad="26"/>
<connect gate="G$1" pin="DCOM" pad="16"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="RANGE" pad="2"/>
<connect gate="G$1" pin="RANGE@1" pad="3"/>
<connect gate="G$1" pin="REFIN" pad="7"/>
<connect gate="G$1" pin="REFOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DAC813AU"/>
<attribute name="OC_FARNELL" value="1509910"/>
<attribute name="OC_NEWARK" value="74C9290"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!LDAC" pad="12"/>
<connect gate="G$1" pin="!LLSB" pad="15"/>
<connect gate="G$1" pin="!LMSB" pad="14"/>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="!WR" pad="11"/>
<connect gate="G$1" pin="+VCC" pad="8"/>
<connect gate="G$1" pin="+VL" pad="1"/>
<connect gate="G$1" pin="-VCC" pad="10"/>
<connect gate="G$1" pin="ACOM" pad="5"/>
<connect gate="G$1" pin="BPO" pad="4"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="18"/>
<connect gate="G$1" pin="D10" pad="27"/>
<connect gate="G$1" pin="D11" pad="28"/>
<connect gate="G$1" pin="D2" pad="19"/>
<connect gate="G$1" pin="D3" pad="20"/>
<connect gate="G$1" pin="D4" pad="21"/>
<connect gate="G$1" pin="D5" pad="22"/>
<connect gate="G$1" pin="D6" pad="23"/>
<connect gate="G$1" pin="D7" pad="24"/>
<connect gate="G$1" pin="D8" pad="25"/>
<connect gate="G$1" pin="D9" pad="26"/>
<connect gate="G$1" pin="DCOM" pad="16"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="RANGE" pad="2"/>
<connect gate="G$1" pin="RANGE@1" pad="3"/>
<connect gate="G$1" pin="REFIN" pad="7"/>
<connect gate="G$1" pin="REFOUT" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DAC813JP"/>
<attribute name="OC_FARNELL" value="1295977"/>
<attribute name="OC_NEWARK" value="61M5756"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC4813" prefix="IC">
<description>&lt;b&gt;Quad 12-Bit DAC&lt;/b&gt;&lt;p&gt;
12-bit port Interface</description>
<gates>
<gate name="G$1" symbol="DAC4813"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!LDAC" pad="19"/>
<connect gate="G$1" pin="!RESET" pad="13"/>
<connect gate="G$1" pin="!WR" pad="14"/>
<connect gate="G$1" pin="+VCC" pad="23"/>
<connect gate="G$1" pin="-VCC" pad="21"/>
<connect gate="G$1" pin="ACOM" pad="22"/>
<connect gate="G$1" pin="DB0" pad="12"/>
<connect gate="G$1" pin="DB1" pad="11"/>
<connect gate="G$1" pin="DB10" pad="2"/>
<connect gate="G$1" pin="DB11" pad="1"/>
<connect gate="G$1" pin="DB2" pad="10"/>
<connect gate="G$1" pin="DB3" pad="9"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="7"/>
<connect gate="G$1" pin="DB6" pad="6"/>
<connect gate="G$1" pin="DB7" pad="5"/>
<connect gate="G$1" pin="DB8" pad="4"/>
<connect gate="G$1" pin="DB9" pad="3"/>
<connect gate="G$1" pin="DCOM" pad="20"/>
<connect gate="G$1" pin="EN1" pad="15"/>
<connect gate="G$1" pin="EN2" pad="16"/>
<connect gate="G$1" pin="EN3" pad="17"/>
<connect gate="G$1" pin="EN4" pad="18"/>
<connect gate="G$1" pin="OUT1" pad="27"/>
<connect gate="G$1" pin="OUT2" pad="26"/>
<connect gate="G$1" pin="OUT3" pad="25"/>
<connect gate="G$1" pin="OUT4" pad="24"/>
<connect gate="G$1" pin="REFOUT" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC7800" prefix="IC">
<description>&lt;b&gt;Dual Monolithic CMOS 12-Bit  DAC&lt;/b&gt;&lt;p&gt; Multiplying</description>
<gates>
<gate name="G$1" symbol="DAC7800"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!CLR" pad="11"/>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="!UPDA" pad="6"/>
<connect gate="G$1" pin="!UPDB" pad="10"/>
<connect gate="G$1" pin="AGNDA" pad="1"/>
<connect gate="G$1" pin="AGNDB" pad="16"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="FBA" pad="3"/>
<connect gate="G$1" pin="FBB" pad="14"/>
<connect gate="G$1" pin="IN" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="15"/>
<connect gate="G$1" pin="REFA" pad="4"/>
<connect gate="G$1" pin="REFB" pad="13"/>
<connect gate="G$1" pin="VDD" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DAC7800LPG4"/>
<attribute name="OC_FARNELL" value="1509905"/>
<attribute name="OC_NEWARK" value="99K1851"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="!CLR" pad="11"/>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="!UPDA" pad="6"/>
<connect gate="G$1" pin="!UPDB" pad="10"/>
<connect gate="G$1" pin="AGNDA" pad="1"/>
<connect gate="G$1" pin="AGNDB" pad="16"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="FBA" pad="3"/>
<connect gate="G$1" pin="FBB" pad="14"/>
<connect gate="G$1" pin="IN" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="15"/>
<connect gate="G$1" pin="REFA" pad="4"/>
<connect gate="G$1" pin="REFB" pad="13"/>
<connect gate="G$1" pin="VDD" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DAC7800KU"/>
<attribute name="OC_FARNELL" value="1460233"/>
<attribute name="OC_NEWARK" value="61M5746"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC7801" prefix="IC">
<description>&lt;b&gt;Dual Monolithic CMOS 12-Bit DAC&lt;/b&gt;&lt;p&gt; Multiplying</description>
<gates>
<gate name="G$1" symbol="DAC7801"/>
</gates>
<devices>
<device name="P" package="DIL24-3">
<connects>
<connect gate="G$1" pin="!CLR" pad="17"/>
<connect gate="G$1" pin="!CS" pad="5"/>
<connect gate="G$1" pin="!UPD" pad="19"/>
<connect gate="G$1" pin="!WR" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="AGNDA" pad="1"/>
<connect gate="G$1" pin="AGNDB" pad="24"/>
<connect gate="G$1" pin="DB0" pad="6"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB2" pad="8"/>
<connect gate="G$1" pin="DB3" pad="9"/>
<connect gate="G$1" pin="DB4" pad="10"/>
<connect gate="G$1" pin="DB5" pad="11"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="FBA" pad="3"/>
<connect gate="G$1" pin="FBB" pad="22"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="23"/>
<connect gate="G$1" pin="REFA" pad="4"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="DAC7801KP"/>
<attribute name="OC_FARNELL" value="1460235"/>
<attribute name="OC_NEWARK" value="14M8160"/>
</technology>
</technologies>
</device>
<device name="U" package="SO24L">
<connects>
<connect gate="G$1" pin="!CLR" pad="17"/>
<connect gate="G$1" pin="!CS" pad="5"/>
<connect gate="G$1" pin="!UPD" pad="19"/>
<connect gate="G$1" pin="!WR" pad="18"/>
<connect gate="G$1" pin="A0" pad="15"/>
<connect gate="G$1" pin="A1" pad="16"/>
<connect gate="G$1" pin="AGNDA" pad="1"/>
<connect gate="G$1" pin="AGNDB" pad="24"/>
<connect gate="G$1" pin="DB0" pad="6"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB2" pad="8"/>
<connect gate="G$1" pin="DB3" pad="9"/>
<connect gate="G$1" pin="DB4" pad="10"/>
<connect gate="G$1" pin="DB5" pad="11"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="FBA" pad="3"/>
<connect gate="G$1" pin="FBB" pad="22"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="23"/>
<connect gate="G$1" pin="REFA" pad="4"/>
<connect gate="G$1" pin="REFB" pad="21"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DAC7801KU"/>
<attribute name="OC_FARNELL" value="1460236"/>
<attribute name="OC_NEWARK" value="61M5748"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC7802" prefix="IC">
<description>&lt;b&gt;Dual Monolithic CMOS 12-Bit DAC&lt;/b&gt;&lt;p&gt;
Multiplying</description>
<gates>
<gate name="G$1" symbol="DAC7802"/>
</gates>
<devices>
<device name="P" package="DIL24-3">
<connects>
<connect gate="G$1" pin="!CSA" pad="5"/>
<connect gate="G$1" pin="!CSB" pad="20"/>
<connect gate="G$1" pin="!WR" pad="19"/>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="DB0" pad="6"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB10" pad="17"/>
<connect gate="G$1" pin="DB11" pad="18"/>
<connect gate="G$1" pin="DB2" pad="8"/>
<connect gate="G$1" pin="DB3" pad="9"/>
<connect gate="G$1" pin="DB4" pad="10"/>
<connect gate="G$1" pin="DB5" pad="11"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="DB8" pad="15"/>
<connect gate="G$1" pin="DB9" pad="16"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="FBA" pad="3"/>
<connect gate="G$1" pin="FBB" pad="23"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="24"/>
<connect gate="G$1" pin="REFA" pad="4"/>
<connect gate="G$1" pin="REFB" pad="22"/>
<connect gate="G$1" pin="VDD" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DAC7802KP"/>
<attribute name="OC_FARNELL" value="1460240"/>
<attribute name="OC_NEWARK" value="61M5750"/>
</technology>
</technologies>
</device>
<device name="U" package="SO24L">
<connects>
<connect gate="G$1" pin="!CSA" pad="5"/>
<connect gate="G$1" pin="!CSB" pad="20"/>
<connect gate="G$1" pin="!WR" pad="19"/>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="DB0" pad="6"/>
<connect gate="G$1" pin="DB1" pad="7"/>
<connect gate="G$1" pin="DB10" pad="17"/>
<connect gate="G$1" pin="DB11" pad="18"/>
<connect gate="G$1" pin="DB2" pad="8"/>
<connect gate="G$1" pin="DB3" pad="9"/>
<connect gate="G$1" pin="DB4" pad="10"/>
<connect gate="G$1" pin="DB5" pad="11"/>
<connect gate="G$1" pin="DB6" pad="13"/>
<connect gate="G$1" pin="DB7" pad="14"/>
<connect gate="G$1" pin="DB8" pad="15"/>
<connect gate="G$1" pin="DB9" pad="16"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="FBA" pad="3"/>
<connect gate="G$1" pin="FBB" pad="23"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="24"/>
<connect gate="G$1" pin="REFA" pad="4"/>
<connect gate="G$1" pin="REFB" pad="22"/>
<connect gate="G$1" pin="VDD" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DAC7802KU"/>
<attribute name="OC_FARNELL" value="1295976"/>
<attribute name="OC_NEWARK" value="74C9283"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA141" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&lt;p&gt;
Precision, Low Power, G = 10, 100</description>
<gates>
<gate name="G$1" symbol="INA141"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="J" pad="1"/>
<connect gate="G$1" pin="J@1" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="J" pad="1"/>
<connect gate="G$1" pin="J@1" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA141U"/>
<attribute name="OC_FARNELL" value="1212419"/>
<attribute name="OC_NEWARK" value="80K5907"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCP0124P" prefix="IC">
<description>&lt;b&gt;DC/DC Converters&lt;/b&gt;&lt;p&gt;
Miniature 24V Input, 1W Isolated Unregulated</description>
<gates>
<gate name="G$1" symbol="DCP0124"/>
</gates>
<devices>
<device name="" package="DIL14/7">
<connects>
<connect gate="G$1" pin="+VOUT" pad="6"/>
<connect gate="G$1" pin="0V" pad="2"/>
<connect gate="G$1" pin="0V@1" pad="5"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="SYIN" pad="14"/>
<connect gate="G$1" pin="SYOUT" pad="8"/>
<connect gate="G$1" pin="VS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DCP012415DBP-U"/>
<attribute name="OC_FARNELL" value="1247063"/>
<attribute name="OC_NEWARK" value="76K4235"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCP0124" prefix="IC">
<description>&lt;b&gt;DC/DC Converters&lt;/b&gt;&lt;p&gt;
Miniature 24V Input, 1W Isolated Unregulated</description>
<gates>
<gate name="G$1" symbol="DCP0124D"/>
</gates>
<devices>
<device name="D" package="DIL14/7">
<connects>
<connect gate="G$1" pin="+VOUT" pad="6"/>
<connect gate="G$1" pin="-VOUT" pad="7"/>
<connect gate="G$1" pin="0V" pad="2"/>
<connect gate="G$1" pin="0V@1" pad="5"/>
<connect gate="G$1" pin="SYIN" pad="14"/>
<connect gate="G$1" pin="SYOUT" pad="8"/>
<connect gate="G$1" pin="VS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DCP012415DBP-U"/>
<attribute name="OC_FARNELL" value="1247063"/>
<attribute name="OC_NEWARK" value="76K4235"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCP0115" prefix="IC">
<description>&lt;b&gt;DC/DC Converters&lt;/b&gt;&lt;p&gt;
Miniature 15V Input, 1W Isolated Unregulated</description>
<gates>
<gate name="G$1" symbol="DCP0124D"/>
</gates>
<devices>
<device name="P" package="DIL14/7">
<connects>
<connect gate="G$1" pin="+VOUT" pad="6"/>
<connect gate="G$1" pin="-VOUT" pad="7"/>
<connect gate="G$1" pin="0V" pad="2"/>
<connect gate="G$1" pin="0V@1" pad="5"/>
<connect gate="G$1" pin="SYIN" pad="14"/>
<connect gate="G$1" pin="SYOUT" pad="8"/>
<connect gate="G$1" pin="VS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="DCP011512DBP"/>
<attribute name="OC_FARNELL" value="1461019"/>
<attribute name="OC_NEWARK" value="74K3725"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DCP0105" prefix="IC">
<description>&lt;b&gt;DC/DC Converters&lt;/b&gt;&lt;p&gt;
Miniature 5V Input, 1W Isolated Unregulated</description>
<gates>
<gate name="G$1" symbol="DCP0124"/>
</gates>
<devices>
<device name="P" package="DIL14/7">
<connects>
<connect gate="G$1" pin="+VOUT" pad="6"/>
<connect gate="G$1" pin="0V" pad="2"/>
<connect gate="G$1" pin="0V@1" pad="5"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="SYIN" pad="14"/>
<connect gate="G$1" pin="SYOUT" pad="8"/>
<connect gate="G$1" pin="VS" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DCP010512BP-U"/>
<attribute name="OC_FARNELL" value="1461015"/>
<attribute name="OC_NEWARK" value="61M5777"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTR103" prefix="IC">
<description>&lt;b&gt;4-20mA Current Transmitter&lt;/b&gt;&lt;p&gt;
with RTD Excitation And Linearization</description>
<gates>
<gate name="G$1" symbol="XTR103"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+IN" pad="4"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="B" pad="15"/>
<connect gate="G$1" pin="E" pad="11"/>
<connect gate="G$1" pin="EINT" pad="14"/>
<connect gate="G$1" pin="IR1" pad="12"/>
<connect gate="G$1" pin="IR2" pad="13"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="RG" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="6"/>
<connect gate="G$1" pin="RLIN" pad="8"/>
<connect gate="G$1" pin="RLIN@1" pad="9"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="ZA" pad="1"/>
<connect gate="G$1" pin="ZA@1" pad="2"/>
<connect gate="G$1" pin="ZA@2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+IN" pad="4"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="B" pad="15"/>
<connect gate="G$1" pin="E" pad="11"/>
<connect gate="G$1" pin="EINT" pad="14"/>
<connect gate="G$1" pin="IR1" pad="12"/>
<connect gate="G$1" pin="IR2" pad="13"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="RG" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="6"/>
<connect gate="G$1" pin="RLIN" pad="8"/>
<connect gate="G$1" pin="RLIN@1" pad="9"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="ZA" pad="1"/>
<connect gate="G$1" pin="ZA@1" pad="2"/>
<connect gate="G$1" pin="ZA@2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTR104" prefix="IC">
<description>&lt;b&gt;4-20mA Current Transmitter&lt;/b&gt;&lt;p&gt;
with Bridge Excitation And Linearization</description>
<gates>
<gate name="G$1" symbol="XTR104"/>
</gates>
<devices>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+LIN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-LIN" pad="4"/>
<connect gate="G$1" pin="B" pad="13"/>
<connect gate="G$1" pin="E" pad="11"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="RG" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="6"/>
<connect gate="G$1" pin="RLIN" pad="8"/>
<connect gate="G$1" pin="RLIN@1" pad="9"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="VREF" pad="12"/>
<connect gate="G$1" pin="ZA" pad="14"/>
<connect gate="G$1" pin="ZA@1" pad="15"/>
<connect gate="G$1" pin="ZA@2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+LIN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="-LIN" pad="4"/>
<connect gate="G$1" pin="B" pad="13"/>
<connect gate="G$1" pin="E" pad="11"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="RG" pad="5"/>
<connect gate="G$1" pin="RG@1" pad="6"/>
<connect gate="G$1" pin="RLIN" pad="8"/>
<connect gate="G$1" pin="RLIN@1" pad="9"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="VREF" pad="12"/>
<connect gate="G$1" pin="ZA" pad="14"/>
<connect gate="G$1" pin="ZA@1" pad="15"/>
<connect gate="G$1" pin="ZA@2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTR105" prefix="IC">
<description>&lt;b&gt;4-20mA Current Transmitter&lt;/b&gt;&lt;p&gt;
with Sensor Excitation and Linearization</description>
<gates>
<gate name="G$1" symbol="XTR105"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="G$1" pin="+IN" pad="13"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="E" pad="8"/>
<connect gate="G$1" pin="IR1" pad="1"/>
<connect gate="G$1" pin="IR2" pad="14"/>
<connect gate="G$1" pin="IRET" pad="6"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="RG" pad="3"/>
<connect gate="G$1" pin="RG@1" pad="4"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="VLIN" pad="12"/>
<connect gate="G$1" pin="VREG" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="XTR105P"/>
<attribute name="OC_FARNELL" value="1461141"/>
<attribute name="OC_NEWARK" value="77C3629"/>
</technology>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="G$1" pin="+IN" pad="13"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="E" pad="8"/>
<connect gate="G$1" pin="IR1" pad="1"/>
<connect gate="G$1" pin="IR2" pad="14"/>
<connect gate="G$1" pin="IRET" pad="6"/>
<connect gate="G$1" pin="NC" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="RG" pad="3"/>
<connect gate="G$1" pin="RG@1" pad="4"/>
<connect gate="G$1" pin="V+" pad="10"/>
<connect gate="G$1" pin="VLIN" pad="12"/>
<connect gate="G$1" pin="VREG" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="XTR105U"/>
<attribute name="OC_FARNELL" value="1212353"/>
<attribute name="OC_NEWARK" value="33C4287"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS901" prefix="IC">
<description>&lt;b&gt;10-Bit, 20 MSPS ADC SE/Diff Inputs&lt;/b&gt;&lt;p&gt;
Ext Reference and Adjustable Fullscale Range</description>
<gates>
<gate name="G$1" symbol="ADS901"/>
</gates>
<devices>
<device name="E" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!OE" pad="16"/>
<connect gate="G$1" pin="+VS" pad="1"/>
<connect gate="G$1" pin="+VS@1" pad="18"/>
<connect gate="G$1" pin="+VS@2" pad="28"/>
<connect gate="G$1" pin="B1" pad="12"/>
<connect gate="G$1" pin="B10" pad="3"/>
<connect gate="G$1" pin="B2" pad="11"/>
<connect gate="G$1" pin="B3" pad="10"/>
<connect gate="G$1" pin="B4" pad="9"/>
<connect gate="G$1" pin="B5" pad="8"/>
<connect gate="G$1" pin="B6" pad="7"/>
<connect gate="G$1" pin="B7" pad="6"/>
<connect gate="G$1" pin="B8" pad="5"/>
<connect gate="G$1" pin="B9" pad="4"/>
<connect gate="G$1" pin="CLK" pad="15"/>
<connect gate="G$1" pin="CM" pad="26"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="20"/>
<connect gate="G$1" pin="IN" pad="27"/>
<connect gate="G$1" pin="LNBY" pad="25"/>
<connect gate="G$1" pin="LPBY" pad="21"/>
<connect gate="G$1" pin="LVDD" pad="2"/>
<connect gate="G$1" pin="NC" pad="23"/>
<connect gate="G$1" pin="PWRD" pad="17"/>
<connect gate="G$1" pin="REFB" pad="24"/>
<connect gate="G$1" pin="REFT" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS901E"/>
<attribute name="OC_FARNELL" value="1509526"/>
<attribute name="OC_NEWARK" value="35C1591"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS574" prefix="IC">
<description>&lt;b&gt;Sampling CMOS A/D Converter&lt;/b&gt;&lt;p&gt;
Microprocessor-Compatible</description>
<gates>
<gate name="G$1" symbol="ADS574"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="10VR" pad="13"/>
<connect gate="G$1" pin="12/!8" pad="2"/>
<connect gate="G$1" pin="20VR" pad="14"/>
<connect gate="G$1" pin="ACOM" pad="9"/>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="BO" pad="12"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="DB0" pad="16"/>
<connect gate="G$1" pin="DB1" pad="17"/>
<connect gate="G$1" pin="DB10" pad="26"/>
<connect gate="G$1" pin="DB11" pad="27"/>
<connect gate="G$1" pin="DB2" pad="18"/>
<connect gate="G$1" pin="DB3" pad="19"/>
<connect gate="G$1" pin="DB4" pad="20"/>
<connect gate="G$1" pin="DB5" pad="21"/>
<connect gate="G$1" pin="DB6" pad="22"/>
<connect gate="G$1" pin="DB7" pad="23"/>
<connect gate="G$1" pin="DB8" pad="24"/>
<connect gate="G$1" pin="DB9" pad="25"/>
<connect gate="G$1" pin="DCOM" pad="15"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="R/!C" pad="5"/>
<connect gate="G$1" pin="REFIN" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="8"/>
<connect gate="G$1" pin="STATUS" pad="28"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS574JP"/>
<attribute name="OC_FARNELL" value="1311734"/>
<attribute name="OC_NEWARK" value="88K1031"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="10VR" pad="13"/>
<connect gate="G$1" pin="12/!8" pad="2"/>
<connect gate="G$1" pin="20VR" pad="14"/>
<connect gate="G$1" pin="ACOM" pad="9"/>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="BO" pad="12"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="DB0" pad="16"/>
<connect gate="G$1" pin="DB1" pad="17"/>
<connect gate="G$1" pin="DB10" pad="26"/>
<connect gate="G$1" pin="DB11" pad="27"/>
<connect gate="G$1" pin="DB2" pad="18"/>
<connect gate="G$1" pin="DB3" pad="19"/>
<connect gate="G$1" pin="DB4" pad="20"/>
<connect gate="G$1" pin="DB5" pad="21"/>
<connect gate="G$1" pin="DB6" pad="22"/>
<connect gate="G$1" pin="DB7" pad="23"/>
<connect gate="G$1" pin="DB8" pad="24"/>
<connect gate="G$1" pin="DB9" pad="25"/>
<connect gate="G$1" pin="DCOM" pad="15"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="R/!C" pad="5"/>
<connect gate="G$1" pin="REFIN" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="8"/>
<connect gate="G$1" pin="STATUS" pad="28"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="JE" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="10VR" pad="13"/>
<connect gate="G$1" pin="12/!8" pad="2"/>
<connect gate="G$1" pin="20VR" pad="14"/>
<connect gate="G$1" pin="ACOM" pad="9"/>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="BO" pad="12"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="DB0" pad="27"/>
<connect gate="G$1" pin="DB1" pad="26"/>
<connect gate="G$1" pin="DB10" pad="17"/>
<connect gate="G$1" pin="DB11" pad="16"/>
<connect gate="G$1" pin="DB2" pad="25"/>
<connect gate="G$1" pin="DB3" pad="24"/>
<connect gate="G$1" pin="DB4" pad="23"/>
<connect gate="G$1" pin="DB5" pad="22"/>
<connect gate="G$1" pin="DB6" pad="21"/>
<connect gate="G$1" pin="DB7" pad="20"/>
<connect gate="G$1" pin="DB8" pad="19"/>
<connect gate="G$1" pin="DB9" pad="18"/>
<connect gate="G$1" pin="DCOM" pad="15"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="R/!C" pad="5"/>
<connect gate="G$1" pin="REFIN" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="8"/>
<connect gate="G$1" pin="STATUS" pad="28"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS574JE"/>
<attribute name="OC_FARNELL" value="1214401"/>
<attribute name="OC_NEWARK" value="01M6815"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS774" prefix="IC">
<description>&lt;b&gt;Sampling CMOS A/D Converter&lt;/b&gt;&lt;p&gt;
Microprocessor Compatible</description>
<gates>
<gate name="G$1" symbol="ADS574"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="10VR" pad="13"/>
<connect gate="G$1" pin="12/!8" pad="2"/>
<connect gate="G$1" pin="20VR" pad="14"/>
<connect gate="G$1" pin="ACOM" pad="9"/>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="BO" pad="12"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="DB0" pad="16"/>
<connect gate="G$1" pin="DB1" pad="17"/>
<connect gate="G$1" pin="DB10" pad="26"/>
<connect gate="G$1" pin="DB11" pad="27"/>
<connect gate="G$1" pin="DB2" pad="18"/>
<connect gate="G$1" pin="DB3" pad="19"/>
<connect gate="G$1" pin="DB4" pad="20"/>
<connect gate="G$1" pin="DB5" pad="21"/>
<connect gate="G$1" pin="DB6" pad="22"/>
<connect gate="G$1" pin="DB7" pad="23"/>
<connect gate="G$1" pin="DB8" pad="24"/>
<connect gate="G$1" pin="DB9" pad="25"/>
<connect gate="G$1" pin="DCOM" pad="15"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="R/!C" pad="5"/>
<connect gate="G$1" pin="REFIN" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="8"/>
<connect gate="G$1" pin="STATUS" pad="28"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS774JP"/>
<attribute name="OC_FARNELL" value="1287416"/>
<attribute name="OC_NEWARK" value="74C7052"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="10VR" pad="13"/>
<connect gate="G$1" pin="12/!8" pad="2"/>
<connect gate="G$1" pin="20VR" pad="14"/>
<connect gate="G$1" pin="ACOM" pad="9"/>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="BO" pad="12"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="DB0" pad="16"/>
<connect gate="G$1" pin="DB1" pad="17"/>
<connect gate="G$1" pin="DB10" pad="26"/>
<connect gate="G$1" pin="DB11" pad="27"/>
<connect gate="G$1" pin="DB2" pad="18"/>
<connect gate="G$1" pin="DB3" pad="19"/>
<connect gate="G$1" pin="DB4" pad="20"/>
<connect gate="G$1" pin="DB5" pad="21"/>
<connect gate="G$1" pin="DB6" pad="22"/>
<connect gate="G$1" pin="DB7" pad="23"/>
<connect gate="G$1" pin="DB8" pad="24"/>
<connect gate="G$1" pin="DB9" pad="25"/>
<connect gate="G$1" pin="DCOM" pad="15"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="R/!C" pad="5"/>
<connect gate="G$1" pin="REFIN" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="8"/>
<connect gate="G$1" pin="STATUS" pad="28"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS774JU"/>
<attribute name="OC_FARNELL" value="1287417"/>
<attribute name="OC_NEWARK" value="25M7542"/>
</technology>
</technologies>
</device>
<device name="JE" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="10VR" pad="13"/>
<connect gate="G$1" pin="12/!8" pad="2"/>
<connect gate="G$1" pin="20VR" pad="14"/>
<connect gate="G$1" pin="ACOM" pad="9"/>
<connect gate="G$1" pin="AO" pad="4"/>
<connect gate="G$1" pin="BO" pad="12"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="DB0" pad="16"/>
<connect gate="G$1" pin="DB1" pad="17"/>
<connect gate="G$1" pin="DB10" pad="26"/>
<connect gate="G$1" pin="DB11" pad="27"/>
<connect gate="G$1" pin="DB2" pad="18"/>
<connect gate="G$1" pin="DB3" pad="19"/>
<connect gate="G$1" pin="DB4" pad="20"/>
<connect gate="G$1" pin="DB5" pad="21"/>
<connect gate="G$1" pin="DB6" pad="22"/>
<connect gate="G$1" pin="DB7" pad="23"/>
<connect gate="G$1" pin="DB8" pad="24"/>
<connect gate="G$1" pin="DB9" pad="25"/>
<connect gate="G$1" pin="DCOM" pad="15"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="R/!C" pad="5"/>
<connect gate="G$1" pin="REFIN" pad="10"/>
<connect gate="G$1" pin="REFOUT" pad="8"/>
<connect gate="G$1" pin="STATUS" pad="28"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VEE" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS774JE"/>
<attribute name="OC_FARNELL" value="1509506"/>
<attribute name="OC_NEWARK" value="74C7051"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7800" prefix="IC">
<description>&lt;b&gt;12-Bit 3us Sampling ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7800"/>
</gates>
<devices>
<device name="U" package="SO28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="21"/>
<connect gate="G$1" pin="!CS" pad="20"/>
<connect gate="G$1" pin="-VS" pad="22"/>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D10" pad="6"/>
<connect gate="G$1" pin="D11" pad="5"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="14"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="7"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="HBE" pad="18"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="R/!C" pad="19"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VSA" pad="24"/>
<connect gate="G$1" pin="VSD" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="21"/>
<connect gate="G$1" pin="!CS" pad="20"/>
<connect gate="G$1" pin="-VS" pad="22"/>
<connect gate="G$1" pin="AGND" pad="4"/>
<connect gate="G$1" pin="D0" pad="17"/>
<connect gate="G$1" pin="D1" pad="16"/>
<connect gate="G$1" pin="D10" pad="6"/>
<connect gate="G$1" pin="D11" pad="5"/>
<connect gate="G$1" pin="D2" pad="15"/>
<connect gate="G$1" pin="D3" pad="14"/>
<connect gate="G$1" pin="D4" pad="12"/>
<connect gate="G$1" pin="D5" pad="11"/>
<connect gate="G$1" pin="D6" pad="10"/>
<connect gate="G$1" pin="D7" pad="9"/>
<connect gate="G$1" pin="D8" pad="8"/>
<connect gate="G$1" pin="D9" pad="7"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="HBE" pad="18"/>
<connect gate="G$1" pin="IN1" pad="1"/>
<connect gate="G$1" pin="IN2" pad="2"/>
<connect gate="G$1" pin="R/!C" pad="19"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VSA" pad="24"/>
<connect gate="G$1" pin="VSD" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACF2101" prefix="IC">
<description>&lt;b&gt;Dual Switched Integrator&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ACF2101"/>
</gates>
<devices>
<device name="P" package="DIL24-3">
<connects>
<connect gate="G$1" pin="CAPA" pad="4"/>
<connect gate="G$1" pin="CAPB" pad="9"/>
<connect gate="G$1" pin="COMA" pad="3"/>
<connect gate="G$1" pin="COMB" pad="10"/>
<connect gate="G$1" pin="GNDA" pad="2"/>
<connect gate="G$1" pin="GNDB" pad="11"/>
<connect gate="G$1" pin="HOLDA" pad="20"/>
<connect gate="G$1" pin="HOLDB" pad="17"/>
<connect gate="G$1" pin="INA" pad="5"/>
<connect gate="G$1" pin="INB" pad="8"/>
<connect gate="G$1" pin="OUTA" pad="1"/>
<connect gate="G$1" pin="OUTB" pad="12"/>
<connect gate="G$1" pin="RESA" pad="21"/>
<connect gate="G$1" pin="RESB" pad="16"/>
<connect gate="G$1" pin="SCOMA" pad="23"/>
<connect gate="G$1" pin="SCOMB" pad="14"/>
<connect gate="G$1" pin="SELA" pad="22"/>
<connect gate="G$1" pin="SELB" pad="15"/>
<connect gate="G$1" pin="SINA" pad="6"/>
<connect gate="G$1" pin="SINB" pad="7"/>
<connect gate="G$1" pin="SOUTA" pad="24"/>
<connect gate="G$1" pin="SOUTB" pad="13"/>
<connect gate="G$1" pin="V+" pad="19"/>
<connect gate="G$1" pin="V-" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO24L">
<connects>
<connect gate="G$1" pin="CAPA" pad="22"/>
<connect gate="G$1" pin="CAPB" pad="3"/>
<connect gate="G$1" pin="COMA" pad="21"/>
<connect gate="G$1" pin="COMB" pad="4"/>
<connect gate="G$1" pin="GNDA" pad="20"/>
<connect gate="G$1" pin="GNDB" pad="5"/>
<connect gate="G$1" pin="HOLDA" pad="14"/>
<connect gate="G$1" pin="HOLDB" pad="11"/>
<connect gate="G$1" pin="INA" pad="23"/>
<connect gate="G$1" pin="INB" pad="2"/>
<connect gate="G$1" pin="OUTA" pad="19"/>
<connect gate="G$1" pin="OUTB" pad="6"/>
<connect gate="G$1" pin="RESA" pad="15"/>
<connect gate="G$1" pin="RESB" pad="10"/>
<connect gate="G$1" pin="SCOMA" pad="17"/>
<connect gate="G$1" pin="SCOMB" pad="8"/>
<connect gate="G$1" pin="SELA" pad="16"/>
<connect gate="G$1" pin="SELB" pad="9"/>
<connect gate="G$1" pin="SINA" pad="24"/>
<connect gate="G$1" pin="SINB" pad="1"/>
<connect gate="G$1" pin="SOUTA" pad="18"/>
<connect gate="G$1" pin="SOUTB" pad="7"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ACF2101BU."/>
<attribute name="OC_FARNELL" value="1206857"/>
<attribute name="OC_NEWARK" value="34R6526"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AFE1103" prefix="IC">
<description>&lt;b&gt;HDSL/MDSL Analog Front End&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AFE1103"/>
</gates>
<devices>
<device name="E" package="SSOP48DL">
<connects>
<connect gate="G$1" pin="AGND" pad="32"/>
<connect gate="G$1" pin="AGND@1" pad="33"/>
<connect gate="G$1" pin="AGND@2" pad="38"/>
<connect gate="G$1" pin="AGND@3" pad="42"/>
<connect gate="G$1" pin="AVDD" pad="27"/>
<connect gate="G$1" pin="AVDD@1" pad="37"/>
<connect gate="G$1" pin="AVDD@2" pad="40"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DGND@1" pad="22"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="NC" pad="43"/>
<connect gate="G$1" pin="NC@1" pad="44"/>
<connect gate="G$1" pin="NC@2" pad="45"/>
<connect gate="G$1" pin="NC@3" pad="46"/>
<connect gate="G$1" pin="PGND" pad="1"/>
<connect gate="G$1" pin="PLLIN" pad="48"/>
<connect gate="G$1" pin="PLLOUT" pad="47"/>
<connect gate="G$1" pin="PVDD" pad="2"/>
<connect gate="G$1" pin="REFN" pad="36"/>
<connect gate="G$1" pin="REFP" pad="34"/>
<connect gate="G$1" pin="RXD0" pad="6"/>
<connect gate="G$1" pin="RXD1" pad="7"/>
<connect gate="G$1" pin="RXD10" pad="18"/>
<connect gate="G$1" pin="RXD11" pad="19"/>
<connect gate="G$1" pin="RXD12" pad="20"/>
<connect gate="G$1" pin="RXD13" pad="21"/>
<connect gate="G$1" pin="RXD2" pad="8"/>
<connect gate="G$1" pin="RXD3" pad="9"/>
<connect gate="G$1" pin="RXD4" pad="10"/>
<connect gate="G$1" pin="RXD5" pad="11"/>
<connect gate="G$1" pin="RXD6" pad="14"/>
<connect gate="G$1" pin="RXD7" pad="15"/>
<connect gate="G$1" pin="RXD8" pad="16"/>
<connect gate="G$1" pin="RXD9" pad="17"/>
<connect gate="G$1" pin="RXGAIN0" pad="24"/>
<connect gate="G$1" pin="RXGAIN1" pad="25"/>
<connect gate="G$1" pin="RXHYBN" pad="28"/>
<connect gate="G$1" pin="RXHYBP" pad="29"/>
<connect gate="G$1" pin="RXLN" pad="39"/>
<connect gate="G$1" pin="RXLOOP" pad="26"/>
<connect gate="G$1" pin="RXLP" pad="31"/>
<connect gate="G$1" pin="RXSYNC" pad="23"/>
<connect gate="G$1" pin="TXCLK" pad="3"/>
<connect gate="G$1" pin="TXDN" pad="4"/>
<connect gate="G$1" pin="TXDP" pad="5"/>
<connect gate="G$1" pin="TXLN" pad="30"/>
<connect gate="G$1" pin="TXLP" pad="41"/>
<connect gate="G$1" pin="VCM" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="AFE1103E"/>
<attribute name="OC_FARNELL" value="1509833"/>
<attribute name="OC_NEWARK" value="74C7270"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DDC101" prefix="IC">
<description>&lt;b&gt;20-Bit ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DDC101U"/>
</gates>
<devices>
<device name="U" package="SO24L">
<connects>
<connect gate="G$1" pin="!DTR" pad="18"/>
<connect gate="G$1" pin="!DVAL" pad="15"/>
<connect gate="G$1" pin="!FDS" pad="8"/>
<connect gate="G$1" pin="!OVF+" pad="17"/>
<connect gate="G$1" pin="!OVF-" pad="16"/>
<connect gate="G$1" pin="!RESE" pad="21"/>
<connect gate="G$1" pin="!RESYS" pad="7"/>
<connect gate="G$1" pin="ANACOM" pad="2"/>
<connect gate="G$1" pin="ANACOM@1" pad="4"/>
<connect gate="G$1" pin="DATACLK" pad="10"/>
<connect gate="G$1" pin="DATAIN" pad="11"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="14"/>
<connect gate="G$1" pin="RD/!SE" pad="19"/>
<connect gate="G$1" pin="REF" pad="23"/>
<connect gate="G$1" pin="REFBB" pad="24"/>
<connect gate="G$1" pin="SETUP" pad="20"/>
<connect gate="G$1" pin="SYSCLK" pad="9"/>
<connect gate="G$1" pin="TEST" pad="22"/>
<connect gate="G$1" pin="VDD+" pad="12"/>
<connect gate="G$1" pin="VS+" pad="5"/>
<connect gate="G$1" pin="VS+@1" pad="6"/>
<connect gate="G$1" pin="VS-" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DDC101U"/>
<attribute name="OC_FARNELL" value="1459305"/>
<attribute name="OC_NEWARK" value="05M6382"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!DTR" pad="20"/>
<connect gate="G$1" pin="!DVAL" pad="17"/>
<connect gate="G$1" pin="!FDS" pad="10"/>
<connect gate="G$1" pin="!OVF+" pad="19"/>
<connect gate="G$1" pin="!OVF-" pad="18"/>
<connect gate="G$1" pin="!RESE" pad="25"/>
<connect gate="G$1" pin="!RESYS" pad="9"/>
<connect gate="G$1" pin="ANACOM" pad="2"/>
<connect gate="G$1" pin="ANACOM@1" pad="4"/>
<connect gate="G$1" pin="DATACLK" pad="12"/>
<connect gate="G$1" pin="DATAIN" pad="13"/>
<connect gate="G$1" pin="DGND" pad="15"/>
<connect gate="G$1" pin="DIN" pad="3"/>
<connect gate="G$1" pin="DOUT" pad="16"/>
<connect gate="G$1" pin="RD/!SE" pad="23"/>
<connect gate="G$1" pin="REF" pad="27"/>
<connect gate="G$1" pin="REFBB" pad="28"/>
<connect gate="G$1" pin="SETUP" pad="24"/>
<connect gate="G$1" pin="SYSCLK" pad="11"/>
<connect gate="G$1" pin="TEST" pad="26"/>
<connect gate="G$1" pin="VDD+" pad="14"/>
<connect gate="G$1" pin="VS+" pad="5"/>
<connect gate="G$1" pin="VS+@1" pad="6"/>
<connect gate="G$1" pin="VS-" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM63P" prefix="IC">
<description>&lt;b&gt;Colinear 20-Bit Monolithic Audio DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCM63P"/>
</gates>
<devices>
<device name="" package="DIL28">
<connects>
<connect gate="G$1" pin="+VA" pad="2"/>
<connect gate="G$1" pin="+VD" pad="13"/>
<connect gate="G$1" pin="-VA" pad="28"/>
<connect gate="G$1" pin="-VD" pad="11"/>
<connect gate="G$1" pin="ACOM" pad="7"/>
<connect gate="G$1" pin="BPO" pad="5"/>
<connect gate="G$1" pin="CLK" pad="18"/>
<connect gate="G$1" pin="DATA" pad="21"/>
<connect gate="G$1" pin="DCOM" pad="12"/>
<connect gate="G$1" pin="IOUT" pad="6"/>
<connect gate="G$1" pin="LB2" pad="24"/>
<connect gate="G$1" pin="LE" pad="20"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="14"/>
<connect gate="G$1" pin="NC@2" pad="15"/>
<connect gate="G$1" pin="NC@3" pad="16"/>
<connect gate="G$1" pin="NC@4" pad="17"/>
<connect gate="G$1" pin="NC@5" pad="19"/>
<connect gate="G$1" pin="NC@6" pad="22"/>
<connect gate="G$1" pin="NC@7" pad="26"/>
<connect gate="G$1" pin="NC@8" pad="27"/>
<connect gate="G$1" pin="OCAP" pad="4"/>
<connect gate="G$1" pin="POT" pad="25"/>
<connect gate="G$1" pin="RCAP" pad="3"/>
<connect gate="G$1" pin="RF1" pad="9"/>
<connect gate="G$1" pin="RF2" pad="10"/>
<connect gate="G$1" pin="SCAP" pad="1"/>
<connect gate="G$1" pin="UB2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA547" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
High-Voltage, High-Current</description>
<gates>
<gate name="G$1" symbol="OPA548"/>
</gates>
<devices>
<device name="F" package="DD-7">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="E/S" pad="7"/>
<connect gate="G$1" pin="ILIM" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OPA547FKTWT.."/>
<attribute name="OC_FARNELL" value="1648714"/>
<attribute name="OC_NEWARK" value="80P7372"/>
</technology>
</technologies>
</device>
<device name="T" package="TO220-7">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="E/S" pad="7"/>
<connect gate="G$1" pin="ILIM" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA547T"/>
<attribute name="OC_FARNELL" value="1564871"/>
<attribute name="OC_NEWARK" value="62K3461"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA544" prefix="IC">
<description>&lt;b&gt;Operational Amplifier&lt;/b&gt;&lt;p&gt;
High-Voltage, High-Current</description>
<gates>
<gate name="G$1" symbol="OP-AMP+-"/>
</gates>
<devices>
<device name="T" package="TO220-G5">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA544T"/>
<attribute name="OC_FARNELL" value="1097575"/>
<attribute name="OC_NEWARK" value="36K2005"/>
</technology>
</technologies>
</device>
<device name="T1" package="TO220-5">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="OPA544T"/>
<attribute name="OC_FARNELL" value="1097575"/>
<attribute name="OC_NEWARK" value="36K2005"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA128" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifiers&lt;/b&gt;&lt;p&gt;
Precision, Low Power</description>
<gates>
<gate name="G$1" symbol="INA128"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA128P"/>
<attribute name="OC_FARNELL" value="1212410"/>
<attribute name="OC_NEWARK" value="74C9783"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA128U"/>
<attribute name="OC_FARNELL" value="1212413"/>
<attribute name="OC_NEWARK" value="35C1729"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA129" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifiers&lt;/b&gt;&lt;p&gt;
Precision, Low Power</description>
<gates>
<gate name="G$1" symbol="INA128"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA129P"/>
<attribute name="OC_FARNELL" value="1212414"/>
<attribute name="OC_NEWARK" value="74C9786"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA129U"/>
<attribute name="OC_FARNELL" value="1212415"/>
<attribute name="OC_NEWARK" value="35C1732"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA134" prefix="IC">
<description>&lt;b&gt;Audio Differential Line Receivers&lt;/b&gt;&lt;p&gt;
0dB, G=1</description>
<gates>
<gate name="G$1" symbol="INA134"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA134PA"/>
<attribute name="OC_FARNELL" value="1247366"/>
<attribute name="OC_NEWARK" value="88K1115"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="INA134UAE4"/>
<attribute name="OC_FARNELL" value="1206899"/>
<attribute name="OC_NEWARK" value="97K1923"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA2134" prefix="IC">
<description>&lt;b&gt;Audio Differential Line Receivers&lt;/b&gt;&lt;p&gt;
0dB, G=1</description>
<gates>
<gate name="G$1" symbol="INA2134"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="G$1" pin="+INA" pad="3"/>
<connect gate="G$1" pin="+INB" pad="5"/>
<connect gate="G$1" pin="-INA" pad="2"/>
<connect gate="G$1" pin="-INB" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="13"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
<connect gate="G$1" pin="REFA" pad="14"/>
<connect gate="G$1" pin="REFB" pad="8"/>
<connect gate="G$1" pin="SENSEA" pad="12"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA2134PA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="14M8174"/>
</technology>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="G$1" pin="+INA" pad="3"/>
<connect gate="G$1" pin="+INB" pad="5"/>
<connect gate="G$1" pin="-INA" pad="2"/>
<connect gate="G$1" pin="-INB" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="13"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
<connect gate="G$1" pin="REFA" pad="14"/>
<connect gate="G$1" pin="REFB" pad="8"/>
<connect gate="G$1" pin="SENSEA" pad="12"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA2134UA"/>
<attribute name="OC_FARNELL" value="1212422"/>
<attribute name="OC_NEWARK" value="35C1748"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA122" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Single Supply, MicroPower</description>
<gates>
<gate name="G$1" symbol="INA122"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA122P"/>
<attribute name="OC_FARNELL" value="1459460"/>
<attribute name="OC_NEWARK" value="15M0948"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="INA122U"/>
<attribute name="OC_FARNELL" value="1212407"/>
<attribute name="OC_NEWARK" value="97K1918"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA132" prefix="IC">
<description>&lt;b&gt;Difference Amplifier&lt;/b&gt;&lt;p&gt;
Low Power, Single-Supply</description>
<gates>
<gate name="G$1" symbol="INA134"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA132U"/>
<attribute name="OC_FARNELL" value="1212416"/>
<attribute name="OC_NEWARK" value="35C1734"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA118" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Precision, Low Power</description>
<gates>
<gate name="G$1" symbol="INA118"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA118P"/>
<attribute name="OC_FARNELL" value="1470354"/>
<attribute name="OC_NEWARK" value="96K4515"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA118U"/>
<attribute name="OC_FARNELL" value="1212404"/>
<attribute name="OC_NEWARK" value="04M6168"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA125" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
with Precision Voltage Reference</description>
<gates>
<gate name="G$1" symbol="INA125"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!SLEEP" pad="2"/>
<connect gate="G$1" pin="+IN" pad="6"/>
<connect gate="G$1" pin="-IN" pad="7"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="REF10" pad="16"/>
<connect gate="G$1" pin="REF2.5" pad="14"/>
<connect gate="G$1" pin="REF5" pad="15"/>
<connect gate="G$1" pin="REFBG" pad="13"/>
<connect gate="G$1" pin="REFCOM" pad="12"/>
<connect gate="G$1" pin="REFOUT" pad="4"/>
<connect gate="G$1" pin="RG" pad="8"/>
<connect gate="G$1" pin="RG@1" pad="9"/>
<connect gate="G$1" pin="SENSE" pad="11"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA125P"/>
<attribute name="OC_FARNELL" value="1459461"/>
<attribute name="OC_NEWARK" value="35C1726"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="!SLEEP" pad="2"/>
<connect gate="G$1" pin="+IN" pad="6"/>
<connect gate="G$1" pin="-IN" pad="7"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="REF10" pad="16"/>
<connect gate="G$1" pin="REF2.5" pad="14"/>
<connect gate="G$1" pin="REF5" pad="15"/>
<connect gate="G$1" pin="REFBG" pad="13"/>
<connect gate="G$1" pin="REFCOM" pad="12"/>
<connect gate="G$1" pin="REFOUT" pad="4"/>
<connect gate="G$1" pin="RG" pad="8"/>
<connect gate="G$1" pin="RG@1" pad="9"/>
<connect gate="G$1" pin="SENSE" pad="11"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA125U"/>
<attribute name="OC_FARNELL" value="1304375"/>
<attribute name="OC_NEWARK" value="80K5901"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA117" prefix="IC">
<description>&lt;b&gt;Difference Amplifier&lt;/b&gt;&lt;p&gt;
High Common-Mode Voltage</description>
<gates>
<gate name="G$1" symbol="INA117"/>
</gates>
<devices>
<device name="M" package="TO99">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="1"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="INA117AM"/>
<attribute name="OC_FARNELL" value="1459424"/>
<attribute name="OC_NEWARK" value="61M6784"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="1"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA117P"/>
<attribute name="OC_FARNELL" value="1470350"/>
<attribute name="OC_NEWARK" value="74K3811"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="COMP" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="1"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA117KU"/>
<attribute name="OC_FARNELL" value="1706653"/>
<attribute name="OC_NEWARK" value="17M6717"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA116" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Ultra Low Input Bias Current</description>
<gates>
<gate name="G$1" symbol="INA116"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+IN" pad="6"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="GUARD+" pad="5"/>
<connect gate="G$1" pin="GUARD+@1" pad="7"/>
<connect gate="G$1" pin="GUARD-" pad="2"/>
<connect gate="G$1" pin="GUARD-@1" pad="4"/>
<connect gate="G$1" pin="NC" pad="10"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="14"/>
<connect gate="G$1" pin="NC@3" pad="15"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="9"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="16"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA116PA"/>
<attribute name="OC_FARNELL" value="1231983"/>
<attribute name="OC_NEWARK" value="78K8300"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+IN" pad="6"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="GUARD+" pad="5"/>
<connect gate="G$1" pin="GUARD+@1" pad="7"/>
<connect gate="G$1" pin="GUARD-" pad="2"/>
<connect gate="G$1" pin="GUARD-@1" pad="4"/>
<connect gate="G$1" pin="NC" pad="10"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="14"/>
<connect gate="G$1" pin="NC@3" pad="15"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="9"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="16"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA116UA"/>
<attribute name="OC_FARNELL" value="1212402"/>
<attribute name="OC_NEWARK" value="35C1717"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA114" prefix="IC">
<description>&lt;b&gt;Precision Instrumentation Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="INA114"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA114BP"/>
<attribute name="OC_FARNELL" value="1212399"/>
<attribute name="OC_NEWARK" value="74K3810"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA114U" prefix="IC">
<description>&lt;b&gt;Precision Instrumentation Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="INA114U"/>
</gates>
<devices>
<device name="" package="SO16-1">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="FB" pad="12"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="6"/>
<connect gate="G$1" pin="NC@3" pad="8"/>
<connect gate="G$1" pin="NC@4" pad="9"/>
<connect gate="G$1" pin="NC@5" pad="14"/>
<connect gate="G$1" pin="NC@6" pad="16"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="10"/>
<connect gate="G$1" pin="RG" pad="2"/>
<connect gate="G$1" pin="RG@1" pad="15"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA114BU"/>
<attribute name="OC_FARNELL" value="1212401"/>
<attribute name="OC_NEWARK" value="74C9759"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA111" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
High Speed FET-Input</description>
<gates>
<gate name="G$1" symbol="INA114"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA111BP"/>
<attribute name="OC_FARNELL" value="1212397"/>
<attribute name="OC_NEWARK" value="27C4351"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA111U" prefix="IC">
<description>&lt;b&gt;Precision Instrumentation Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="INA114U"/>
</gates>
<devices>
<device name="" package="SO16-1">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="FB" pad="12"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="3"/>
<connect gate="G$1" pin="NC@2" pad="6"/>
<connect gate="G$1" pin="NC@3" pad="8"/>
<connect gate="G$1" pin="NC@4" pad="9"/>
<connect gate="G$1" pin="NC@5" pad="14"/>
<connect gate="G$1" pin="NC@6" pad="16"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="10"/>
<connect gate="G$1" pin="RG" pad="2"/>
<connect gate="G$1" pin="RG@1" pad="15"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA111BP"/>
<attribute name="OC_FARNELL" value="1212397"/>
<attribute name="OC_NEWARK" value="27C4351"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA103" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Low Distortion, Low Noise</description>
<gates>
<gate name="G$1" symbol="INA103"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+GD" pad="5"/>
<connect gate="G$1" pin="+GS" pad="2"/>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+OFFS" pad="3"/>
<connect gate="G$1" pin="+RG" pad="6"/>
<connect gate="G$1" pin="-GD" pad="12"/>
<connect gate="G$1" pin="-GS" pad="15"/>
<connect gate="G$1" pin="-IN" pad="16"/>
<connect gate="G$1" pin="-OFFS" pad="4"/>
<connect gate="G$1" pin="-RG" pad="13"/>
<connect gate="G$1" pin="G=100" pad="14"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="SENSE" pad="11"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA103KP"/>
<attribute name="OC_FARNELL" value="1212392"/>
<attribute name="OC_NEWARK" value="74K3805"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+GD" pad="5"/>
<connect gate="G$1" pin="+GS" pad="2"/>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="+OFFS" pad="3"/>
<connect gate="G$1" pin="+RG" pad="6"/>
<connect gate="G$1" pin="-GD" pad="12"/>
<connect gate="G$1" pin="-GS" pad="15"/>
<connect gate="G$1" pin="-IN" pad="16"/>
<connect gate="G$1" pin="-OFFS" pad="4"/>
<connect gate="G$1" pin="-RG" pad="13"/>
<connect gate="G$1" pin="G=100" pad="14"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="SENSE" pad="11"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA103KU"/>
<attribute name="OC_FARNELL" value="1212393"/>
<attribute name="OC_NEWARK" value="35C1712"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA137" prefix="IC">
<description>&lt;b&gt;Audio Differential Line Receivers&lt;/b&gt;&lt;p&gt;
+-6dB, G=1/2 or 2</description>
<gates>
<gate name="G$1" symbol="INA134"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA137PA"/>
<attribute name="OC_FARNELL" value="4970305"/>
<attribute name="OC_NEWARK" value="35C0496"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA137UA"/>
<attribute name="OC_FARNELL" value="1212418"/>
<attribute name="OC_NEWARK" value="80K5905"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA2137" prefix="IC">
<description>&lt;b&gt;Audio Differential Line Receivers&lt;/b&gt;&lt;p&gt;
+-6dB, G=1/2 or 2</description>
<gates>
<gate name="G$1" symbol="INA2134"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="G$1" pin="+INA" pad="3"/>
<connect gate="G$1" pin="+INB" pad="5"/>
<connect gate="G$1" pin="-INA" pad="2"/>
<connect gate="G$1" pin="-INB" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="13"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
<connect gate="G$1" pin="REFA" pad="14"/>
<connect gate="G$1" pin="REFB" pad="8"/>
<connect gate="G$1" pin="SENSEA" pad="12"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA2137PA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M9116"/>
</technology>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="G$1" pin="+INA" pad="3"/>
<connect gate="G$1" pin="+INB" pad="5"/>
<connect gate="G$1" pin="-INA" pad="2"/>
<connect gate="G$1" pin="-INB" pad="6"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="13"/>
<connect gate="G$1" pin="OUTB" pad="9"/>
<connect gate="G$1" pin="REFA" pad="14"/>
<connect gate="G$1" pin="REFB" pad="8"/>
<connect gate="G$1" pin="SENSEA" pad="12"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA2137UA"/>
<attribute name="OC_FARNELL" value="1703321"/>
<attribute name="OC_NEWARK" value="35C1749"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA105" prefix="IC">
<description>&lt;b&gt;Precision Unity Gain Diff. Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="INA134"/>
</gates>
<devices>
<device name="M" package="TO99">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA105BM"/>
<attribute name="OC_FARNELL" value="1459423"/>
<attribute name="OC_NEWARK" value="88K1114"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA105KP"/>
<attribute name="OC_FARNELL" value="1651850"/>
<attribute name="OC_NEWARK" value="04M4538"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA105KU"/>
<attribute name="OC_FARNELL" value="1754832"/>
<attribute name="OC_NEWARK" value="35C0475"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA2126" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt; Micropower, Single and Dual Versions&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ina2126.pdf</description>
<gates>
<gate name="G$1" symbol="INA2126"/>
</gates>
<devices>
<device name="E" package="SSOP16BU">
<connects>
<connect gate="G$1" pin="+INA" pad="2"/>
<connect gate="G$1" pin="+INB" pad="15"/>
<connect gate="G$1" pin="-INA" pad="1"/>
<connect gate="G$1" pin="-INB" pad="16"/>
<connect gate="G$1" pin="OUTA" pad="6"/>
<connect gate="G$1" pin="OUTB" pad="11"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="12"/>
<connect gate="G$1" pin="RGA" pad="3"/>
<connect gate="G$1" pin="RGA@1" pad="4"/>
<connect gate="G$1" pin="RGB" pad="14"/>
<connect gate="G$1" pin="RGB@1" pad="13"/>
<connect gate="G$1" pin="SENSEA" pad="7"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="INA2126UAE4"/>
<attribute name="OC_FARNELL" value="1234796"/>
<attribute name="OC_NEWARK" value="13M1604"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+INA" pad="2"/>
<connect gate="G$1" pin="+INB" pad="15"/>
<connect gate="G$1" pin="-INA" pad="1"/>
<connect gate="G$1" pin="-INB" pad="16"/>
<connect gate="G$1" pin="OUTA" pad="6"/>
<connect gate="G$1" pin="OUTB" pad="11"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="12"/>
<connect gate="G$1" pin="RGA" pad="3"/>
<connect gate="G$1" pin="RGA@1" pad="4"/>
<connect gate="G$1" pin="RGB" pad="14"/>
<connect gate="G$1" pin="RGB@1" pad="13"/>
<connect gate="G$1" pin="SENSEA" pad="7"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA2126P"/>
<attribute name="OC_FARNELL" value="1535404"/>
<attribute name="OC_NEWARK" value="74C9838"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16">
<connects>
<connect gate="G$1" pin="+INA" pad="2"/>
<connect gate="G$1" pin="+INB" pad="15"/>
<connect gate="G$1" pin="-INA" pad="1"/>
<connect gate="G$1" pin="-INB" pad="16"/>
<connect gate="G$1" pin="OUTA" pad="6"/>
<connect gate="G$1" pin="OUTB" pad="11"/>
<connect gate="G$1" pin="REFA" pad="5"/>
<connect gate="G$1" pin="REFB" pad="12"/>
<connect gate="G$1" pin="RGA" pad="3"/>
<connect gate="G$1" pin="RGA@1" pad="4"/>
<connect gate="G$1" pin="RGB" pad="14"/>
<connect gate="G$1" pin="RGB@1" pad="13"/>
<connect gate="G$1" pin="SENSEA" pad="7"/>
<connect gate="G$1" pin="SENSEB" pad="10"/>
<connect gate="G$1" pin="V+" pad="9"/>
<connect gate="G$1" pin="V-" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA2126U"/>
<attribute name="OC_FARNELL" value="1459464"/>
<attribute name="OC_NEWARK" value="74C9839"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA126" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Micropower, Single and Dual Versions</description>
<gates>
<gate name="G$1" symbol="INA126"/>
</gates>
<devices>
<device name="E" package="MSOP08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA126E/250"/>
<attribute name="OC_FARNELL" value="1575427"/>
<attribute name="OC_NEWARK" value="74C9777"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="INA126P"/>
<attribute name="OC_FARNELL" value="1509595"/>
<attribute name="OC_NEWARK" value="74C9780"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG" pad="1"/>
<connect gate="G$1" pin="RG@1" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA126U"/>
<attribute name="OC_FARNELL" value="1212409"/>
<attribute name="OC_NEWARK" value="84K8003"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO212P" prefix="IC">
<description>&lt;b&gt;Isolated DC/DC Amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ISO212"/>
</gates>
<devices>
<device name="" package="ZZ326">
<connects>
<connect gate="G$1" pin="+I/P" pad="1"/>
<connect gate="G$1" pin="+VSS1" pad="6"/>
<connect gate="G$1" pin="-I/P" pad="3"/>
<connect gate="G$1" pin="-VSS1" pad="5"/>
<connect gate="G$1" pin="CLKIN" pad="35"/>
<connect gate="G$1" pin="CLKOUT" pad="34"/>
<connect gate="G$1" pin="COM1" pad="2"/>
<connect gate="G$1" pin="COM2" pad="32"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="O/PHIGH" pad="38"/>
<connect gate="G$1" pin="O/PLOW" pad="37"/>
<connect gate="G$1" pin="OFFA" pad="7"/>
<connect gate="G$1" pin="OFFA@1" pad="8"/>
<connect gate="G$1" pin="VCC" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUF634" prefix="IC">
<description>&lt;b&gt;250mA High-Speed Buffer&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BUF634"/>
</gates>
<devices>
<device name="T" package="TO220-G5">
<connects>
<connect gate="G$1" pin="BW" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="BUF634T"/>
<attribute name="OC_FARNELL" value="1207894"/>
<attribute name="OC_NEWARK" value="04M8376"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="BW" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="BUF634P"/>
<attribute name="OC_FARNELL" value="1470343"/>
<attribute name="OC_NEWARK" value="80K5714"/>
</technology>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="BW" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="BUF634U"/>
<attribute name="OC_FARNELL" value="4733617"/>
<attribute name="OC_NEWARK" value="27C6567"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC56" prefix="IC">
<description>&lt;b&gt;16-Bit Resolution DAC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DAC56"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+VL" pad="3"/>
<connect gate="G$1" pin="+VS" pad="16"/>
<connect gate="G$1" pin="-VL" pad="8"/>
<connect gate="G$1" pin="-VS" pad="1"/>
<connect gate="G$1" pin="ACOM" pad="12"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="DATA" pad="7"/>
<connect gate="G$1" pin="IOUT" pad="13"/>
<connect gate="G$1" pin="LCOM" pad="2"/>
<connect gate="G$1" pin="LE" pad="6"/>
<connect gate="G$1" pin="MSBAD" pad="14"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="RF" pad="10"/>
<connect gate="G$1" pin="SJ" pad="11"/>
<connect gate="G$1" pin="TRIM" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="+VL" pad="3"/>
<connect gate="G$1" pin="+VS" pad="16"/>
<connect gate="G$1" pin="-VL" pad="8"/>
<connect gate="G$1" pin="-VS" pad="1"/>
<connect gate="G$1" pin="ACOM" pad="12"/>
<connect gate="G$1" pin="CLK" pad="5"/>
<connect gate="G$1" pin="DATA" pad="7"/>
<connect gate="G$1" pin="IOUT" pad="13"/>
<connect gate="G$1" pin="LCOM" pad="2"/>
<connect gate="G$1" pin="LE" pad="6"/>
<connect gate="G$1" pin="MSBAD" pad="14"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="RF" pad="10"/>
<connect gate="G$1" pin="SJ" pad="11"/>
<connect gate="G$1" pin="TRIM" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REG1118" prefix="IC">
<description>&lt;b&gt;800mA Low Dropout (LDO) Positive Regulator&lt;/b&gt;&lt;p&gt;
with Current Source and Sink Capability</description>
<gates>
<gate name="G$1" symbol="REG1118"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="REG1118-2.85/2K5G4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="14M2185"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO150" prefix="IC">
<description>&lt;b&gt;Dual, Isolated, Bi-Directional Digital Coupler&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ISO150"/>
</gates>
<devices>
<device name="P" package="DIL24/12">
<connects>
<connect gate="G$1" pin="D1A" pad="1"/>
<connect gate="G$1" pin="D1B" pad="12"/>
<connect gate="G$1" pin="D2A" pad="24"/>
<connect gate="G$1" pin="D2B" pad="13"/>
<connect gate="G$1" pin="GA" pad="22"/>
<connect gate="G$1" pin="GB" pad="10"/>
<connect gate="G$1" pin="R/!T1A" pad="2"/>
<connect gate="G$1" pin="R/!T1B" pad="11"/>
<connect gate="G$1" pin="R/!T2A" pad="23"/>
<connect gate="G$1" pin="R/!T2B" pad="14"/>
<connect gate="G$1" pin="VSA" pad="3"/>
<connect gate="G$1" pin="VSB" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="U" package="SO28-3/12">
<connects>
<connect gate="G$1" pin="D1A" pad="1"/>
<connect gate="G$1" pin="D1B" pad="14"/>
<connect gate="G$1" pin="D2A" pad="28"/>
<connect gate="G$1" pin="D2B" pad="15"/>
<connect gate="G$1" pin="GA" pad="26"/>
<connect gate="G$1" pin="GB" pad="12"/>
<connect gate="G$1" pin="R/!T1A" pad="2"/>
<connect gate="G$1" pin="R/!T1B" pad="13"/>
<connect gate="G$1" pin="R/!T2A" pad="27"/>
<connect gate="G$1" pin="R/!T2B" pad="16"/>
<connect gate="G$1" pin="VSA" pad="3"/>
<connect gate="G$1" pin="VSB" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ISO150AUG4"/>
<attribute name="OC_FARNELL" value="1206917"/>
<attribute name="OC_NEWARK" value="40K6952"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7804" prefix="IC">
<description>&lt;b&gt;12-Bit 10us Sampling CMOS ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7804"/>
</gates>
<devices>
<device name="P" package="DIL28-3">
<connects>
<connect gate="G$1" pin="!BUSY" pad="26"/>
<connect gate="G$1" pin="!CS" pad="25"/>
<connect gate="G$1" pin="AGND1" pad="2"/>
<connect gate="G$1" pin="AGND2" pad="5"/>
<connect gate="G$1" pin="B0" pad="22"/>
<connect gate="G$1" pin="B1" pad="21"/>
<connect gate="G$1" pin="B10" pad="11"/>
<connect gate="G$1" pin="B11" pad="10"/>
<connect gate="G$1" pin="B12" pad="9"/>
<connect gate="G$1" pin="B13" pad="8"/>
<connect gate="G$1" pin="B14" pad="7"/>
<connect gate="G$1" pin="B15" pad="6"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="19"/>
<connect gate="G$1" pin="B4" pad="18"/>
<connect gate="G$1" pin="B5" pad="17"/>
<connect gate="G$1" pin="B6" pad="16"/>
<connect gate="G$1" pin="B7" pad="15"/>
<connect gate="G$1" pin="B8" pad="13"/>
<connect gate="G$1" pin="B9" pad="12"/>
<connect gate="G$1" pin="BYTE" pad="23"/>
<connect gate="G$1" pin="CAP" pad="4"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="R/!C" pad="24"/>
<connect gate="G$1" pin="REF" pad="3"/>
<connect gate="G$1" pin="VANA" pad="27"/>
<connect gate="G$1" pin="VDIG" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7804P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="35C1525"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REG1117" prefix="IC">
<description>&lt;b&gt;800mA and 1A Low Dropout (LDO) Positive Regulator&lt;/b&gt;&lt;p&gt;
1.8V, 2.5V, 2.85V, 3.3V, 5V, and Adj</description>
<gates>
<gate name="G$1" symbol="REG1118"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="REG1117"/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="OC_NEWARK" value="14P6981"/>
</technology>
</technologies>
</device>
<device name="F" package="DD-3">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="REG1117FAKTTT"/>
<attribute name="OC_FARNELL" value="1296120"/>
<attribute name="OC_NEWARK" value="87H2562"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7803" prefix="IC">
<description>&lt;b&gt;Autocalibrating, 4-Channel, 12-Bit ADC&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G" symbol="ADS7803"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G" pin="/BUSY" pad="22"/>
<connect gate="G" pin="/CAL" pad="26"/>
<connect gate="G" pin="/CS" pad="19"/>
<connect gate="G" pin="/RD" pad="18"/>
<connect gate="G" pin="/WR" pad="20"/>
<connect gate="G" pin="A0" pad="24"/>
<connect gate="G" pin="A1" pad="25"/>
<connect gate="G" pin="AGND" pad="27"/>
<connect gate="G" pin="AIN0" pad="2"/>
<connect gate="G" pin="AIN1" pad="3"/>
<connect gate="G" pin="AIN2" pad="4"/>
<connect gate="G" pin="AIN3" pad="5"/>
<connect gate="G" pin="CLK" pad="23"/>
<connect gate="G" pin="D0" pad="17"/>
<connect gate="G" pin="D1" pad="16"/>
<connect gate="G" pin="D2" pad="15"/>
<connect gate="G" pin="D3" pad="14"/>
<connect gate="G" pin="D4" pad="13"/>
<connect gate="G" pin="D5" pad="12"/>
<connect gate="G" pin="D6" pad="11"/>
<connect gate="G" pin="D7" pad="10"/>
<connect gate="G" pin="HBE" pad="21"/>
<connect gate="G" pin="SFR" pad="1"/>
<connect gate="G" pin="VD" pad="9"/>
<connect gate="G" pin="VREF+" pad="6"/>
<connect gate="G" pin="VREF-" pad="7"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC7541A" prefix="IC">
<description>&lt;b&gt;Low Cost 12-Bit CMOS DAC&lt;/b&gt; Four-Quadrant Multiplying</description>
<gates>
<gate name="PWR" symbol="PWRN"/>
<gate name="G" symbol="DAC7541A"/>
</gates>
<devices>
<device name="P" package="DIL18">
<connects>
<connect gate="G" pin="B1(MSB)" pad="4"/>
<connect gate="G" pin="B10" pad="13"/>
<connect gate="G" pin="B11" pad="14"/>
<connect gate="G" pin="B12(LSB)" pad="15"/>
<connect gate="G" pin="B2" pad="5"/>
<connect gate="G" pin="B3" pad="6"/>
<connect gate="G" pin="B4" pad="7"/>
<connect gate="G" pin="B5" pad="8"/>
<connect gate="G" pin="B6" pad="9"/>
<connect gate="G" pin="B7" pad="10"/>
<connect gate="G" pin="B8" pad="11"/>
<connect gate="G" pin="B9" pad="12"/>
<connect gate="G" pin="FEEDBACK" pad="18"/>
<connect gate="G" pin="IOUT1" pad="1"/>
<connect gate="G" pin="IOUT2" pad="2"/>
<connect gate="G" pin="VREF" pad="17"/>
<connect gate="PWR" pin="GND" pad="3"/>
<connect gate="PWR" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DAC7541AJP"/>
<attribute name="OC_FARNELL" value="1212269"/>
<attribute name="OC_NEWARK" value="96K4483"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTR110A" prefix="IC">
<description>&lt;b&gt;Precision Voltage-To-Current Converter/Transmitter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="XTR110A"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="16MASPAN" pad="9"/>
<connect gate="G$1" pin="4MASPAN" pad="10"/>
<connect gate="G$1" pin="GATE" pad="14"/>
<connect gate="G$1" pin="OFFSET1" pad="7"/>
<connect gate="G$1" pin="OFFSET2" pad="6"/>
<connect gate="G$1" pin="SPAN" pad="8"/>
<connect gate="G$1" pin="SRES" pad="1"/>
<connect gate="G$1" pin="SSENSE" pad="13"/>
<connect gate="G$1" pin="VIN(10)" pad="4"/>
<connect gate="G$1" pin="VIN(5V)" pad="5"/>
<connect gate="G$1" pin="VREF_IN" pad="3"/>
<connect gate="G$1" pin="V_ADJUST" pad="11"/>
<connect gate="G$1" pin="V_FORCE" pad="15"/>
<connect gate="G$1" pin="V_SENSE" pad="12"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="XTR110AG"/>
<attribute name="OC_FARNELL" value="1652416"/>
<attribute name="OC_NEWARK" value="04M4626"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC7802" prefix="IC" uservalue="yes">
<description>&lt;b&gt;12-Bit Analog to Digital Converter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADC7802"/>
</gates>
<devices>
<device name="PLC" package="PLCC28">
<connects>
<connect gate="G$1" pin="/BUSY" pad="22"/>
<connect gate="G$1" pin="/CAL" pad="26"/>
<connect gate="G$1" pin="/CS" pad="19"/>
<connect gate="G$1" pin="/RD" pad="18"/>
<connect gate="G$1" pin="/WR" pad="20"/>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="25"/>
<connect gate="G$1" pin="AGND" pad="27"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="4"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="CLK" pad="23"/>
<connect gate="G$1" pin="D0/D8" pad="17"/>
<connect gate="G$1" pin="D1/D9" pad="16"/>
<connect gate="G$1" pin="D2/D10" pad="15"/>
<connect gate="G$1" pin="D3/D11" pad="14"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="HBE" pad="21"/>
<connect gate="G$1" pin="SFR" pad="1"/>
<connect gate="G$1" pin="VA" pad="28"/>
<connect gate="G$1" pin="VD" pad="9"/>
<connect gate="G$1" pin="VREF+" pad="6"/>
<connect gate="G$1" pin="VREF-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="PLC-S" package="PLCC-S28">
<connects>
<connect gate="G$1" pin="/BUSY" pad="22"/>
<connect gate="G$1" pin="/CAL" pad="26"/>
<connect gate="G$1" pin="/CS" pad="19"/>
<connect gate="G$1" pin="/RD" pad="18"/>
<connect gate="G$1" pin="/WR" pad="20"/>
<connect gate="G$1" pin="A0" pad="24"/>
<connect gate="G$1" pin="A1" pad="25"/>
<connect gate="G$1" pin="AGND" pad="27"/>
<connect gate="G$1" pin="AIN0" pad="2"/>
<connect gate="G$1" pin="AIN1" pad="3"/>
<connect gate="G$1" pin="AIN2" pad="4"/>
<connect gate="G$1" pin="AIN3" pad="5"/>
<connect gate="G$1" pin="CLK" pad="23"/>
<connect gate="G$1" pin="D0/D8" pad="17"/>
<connect gate="G$1" pin="D1/D9" pad="16"/>
<connect gate="G$1" pin="D2/D10" pad="15"/>
<connect gate="G$1" pin="D3/D11" pad="14"/>
<connect gate="G$1" pin="D4" pad="13"/>
<connect gate="G$1" pin="D5" pad="12"/>
<connect gate="G$1" pin="D6" pad="11"/>
<connect gate="G$1" pin="D7" pad="10"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="HBE" pad="21"/>
<connect gate="G$1" pin="SFR" pad="1"/>
<connect gate="G$1" pin="VA" pad="28"/>
<connect gate="G$1" pin="VD" pad="9"/>
<connect gate="G$1" pin="VREF+" pad="6"/>
<connect gate="G$1" pin="VREF-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO485" prefix="IC">
<description>&lt;b&gt;Isolated RS-485 Differential Bus Transceiver&lt;/b&gt;</description>
<gates>
<gate name="G" symbol="ISO485P"/>
<gate name="A" symbol="PWRN"/>
<gate name="B" symbol="PWR2"/>
</gates>
<devices>
<device name="P" package="DIL24-3/12">
<connects>
<connect gate="A" pin="GND" pad="22"/>
<connect gate="A" pin="VCC" pad="3"/>
<connect gate="B" pin="GND@1" pad="11"/>
<connect gate="B" pin="GND@2" pad="14"/>
<connect gate="B" pin="VCC" pad="15"/>
<connect gate="G" pin="A" pad="12"/>
<connect gate="G" pin="B" pad="13"/>
<connect gate="G" pin="D" pad="24"/>
<connect gate="G" pin="DE" pad="23"/>
<connect gate="G" pin="NC" pad="10"/>
<connect gate="G" pin="R" pad="1"/>
<connect gate="G" pin="RE" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XTR101A" prefix="IC">
<description>&lt;b&gt;Precision, Low Drift 4-20mA Two-Wire Transmitter&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="XTR101A"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="G$1" pin="+IN" pad="4"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="B" pad="12"/>
<connect gate="G$1" pin="BW" pad="13"/>
<connect gate="G$1" pin="E" pad="9"/>
<connect gate="G$1" pin="IREF1" pad="10"/>
<connect gate="G$1" pin="IREF2" pad="11"/>
<connect gate="G$1" pin="OUT" pad="7"/>
<connect gate="G$1" pin="SPAN_0" pad="5"/>
<connect gate="G$1" pin="SPAN_1" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="ZADJ" pad="14"/>
<connect gate="G$1" pin="ZA_0" pad="1"/>
<connect gate="G$1" pin="ZA_1" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="XTR101AP"/>
<attribute name="OC_FARNELL" value="1648756"/>
<attribute name="OC_NEWARK" value="84K4518"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA138" prefix="IC">
<description>&lt;b&gt;High-Side Measurement Current Shunt Monitor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="INA138"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA138NA/250"/>
<attribute name="OC_FARNELL" value="1564888"/>
<attribute name="OC_NEWARK" value="80K5906"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA168" prefix="IC">
<description>&lt;b&gt;High-Side Measurement Current Shunt Monitor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="INA138"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA168NA/250"/>
<attribute name="OC_FARNELL" value="4375737"/>
<attribute name="OC_NEWARK" value="35C1744"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS8344" prefix="IC">
<description>&lt;b&gt;16-Bit, 8-Channel Serial Output Sampling ADC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADS8344"/>
</gates>
<devices>
<device name="U" package="SSOP20BU">
<connects>
<connect gate="G$1" pin="!CS" pad="18"/>
<connect gate="G$1" pin="!SHDN" pad="10"/>
<connect gate="G$1" pin="BUSY" pad="16"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="COM" pad="9"/>
<connect gate="G$1" pin="DCLK" pad="19"/>
<connect gate="G$1" pin="DI" pad="17"/>
<connect gate="G$1" pin="DOUT" pad="15"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VCC@1" pad="20"/>
<connect gate="G$1" pin="VREF" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS8344NB"/>
<attribute name="OC_FARNELL" value="1212294"/>
<attribute name="OC_NEWARK" value="01M6827"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA110*" prefix="IC">
<description>&lt;b&gt;Instrumentation Amplifier&lt;/b&gt;&lt;p&gt;
Fast-Settling FET-Input</description>
<gates>
<gate name="G$1" symbol="INA110"/>
<gate name="P" symbol="+-VCC"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="*10" pad="13"/>
<connect gate="G$1" pin="*100" pad="12"/>
<connect gate="G$1" pin="*200" pad="16"/>
<connect gate="G$1" pin="*500" pad="11"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="OUTPUT" pad="9"/>
<connect gate="G$1" pin="O_IN@1" pad="4"/>
<connect gate="G$1" pin="O_IN@2" pad="5"/>
<connect gate="G$1" pin="O_OUT@1" pad="15"/>
<connect gate="G$1" pin="O_OUT@2" pad="14"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="RG" pad="3"/>
<connect gate="G$1" pin="SENSE" pad="10"/>
<connect gate="P" pin="+VCC" pad="8"/>
<connect gate="P" pin="-VCC" pad="7"/>
</connects>
<technologies>
<technology name="K">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA110KP"/>
<attribute name="OC_FARNELL" value="1097535"/>
<attribute name="OC_NEWARK" value="74K3807"/>
</technology>
</technologies>
</device>
<device name="U" package="SO16-1">
<connects>
<connect gate="G$1" pin="*10" pad="13"/>
<connect gate="G$1" pin="*100" pad="12"/>
<connect gate="G$1" pin="*200" pad="16"/>
<connect gate="G$1" pin="*500" pad="11"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="OUTPUT" pad="9"/>
<connect gate="G$1" pin="O_IN@1" pad="4"/>
<connect gate="G$1" pin="O_IN@2" pad="5"/>
<connect gate="G$1" pin="O_OUT@1" pad="15"/>
<connect gate="G$1" pin="O_OUT@2" pad="14"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="RG" pad="3"/>
<connect gate="G$1" pin="SENSE" pad="10"/>
<connect gate="P" pin="+VCC" pad="8"/>
<connect gate="P" pin="-VCC" pad="7"/>
</connects>
<technologies>
<technology name="K">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA110KU"/>
<attribute name="OC_FARNELL" value="1212396"/>
<attribute name="OC_NEWARK" value="04M4539"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1792" prefix="IC">
<description>&lt;b&gt; AUDIO STEREO DIGITAL-TO-ANALOG CONVERTER&lt;/b&gt; 24-BIT, 192-kHz SAMPLING, ADVANCED SEGMENT&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm1792.pdf</description>
<gates>
<gate name="G$1" symbol="PCM1792"/>
</gates>
<devices>
<device name="" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!MS" pad="10"/>
<connect gate="G$1" pin="!RST" pad="14"/>
<connect gate="G$1" pin="AGND1" pad="19"/>
<connect gate="G$1" pin="AGND2" pad="24"/>
<connect gate="G$1" pin="AGND3L" pad="27"/>
<connect gate="G$1" pin="AGND3R" pad="16"/>
<connect gate="G$1" pin="BCK" pad="6"/>
<connect gate="G$1" pin="DATA" pad="5"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="IOUTL+" pad="25"/>
<connect gate="G$1" pin="IOUTL-" pad="26"/>
<connect gate="G$1" pin="IOUTR+" pad="17"/>
<connect gate="G$1" pin="IOUTR-" pad="18"/>
<connect gate="G$1" pin="IREF" pad="20"/>
<connect gate="G$1" pin="LRCK" pad="4"/>
<connect gate="G$1" pin="MC" pad="12"/>
<connect gate="G$1" pin="MDI" pad="11"/>
<connect gate="G$1" pin="MDO" pad="13"/>
<connect gate="G$1" pin="MSEL" pad="3"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2L" pad="28"/>
<connect gate="G$1" pin="VCC2R" pad="15"/>
<connect gate="G$1" pin="VCOML" pad="22"/>
<connect gate="G$1" pin="VCOMR" pad="21"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="ZEROL" pad="1"/>
<connect gate="G$1" pin="ZEROR" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCM1792DBG4"/>
<attribute name="OC_FARNELL" value="1408321"/>
<attribute name="OC_NEWARK" value="06M7578"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1793" prefix="IC">
<description>&lt;b&gt; AUDIO STEREO DIGITAL-TO-ANALOG CONVERTER&lt;/b&gt; 24-BIT, 192-kHz SAMPLING, ADVANCED SEGMENT&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm1793.pdf</description>
<gates>
<gate name="G$1" symbol="PCM1793"/>
</gates>
<devices>
<device name="" package="SSOP28BU">
<connects>
<connect gate="G$1" pin="!RST" pad="6"/>
<connect gate="G$1" pin="AGNDC" pad="16"/>
<connect gate="G$1" pin="AGNDF" pad="9"/>
<connect gate="G$1" pin="AGNDL" pad="19"/>
<connect gate="G$1" pin="AGNDR" pad="11"/>
<connect gate="G$1" pin="BCK" pad="2"/>
<connect gate="G$1" pin="DATA" pad="3"/>
<connect gate="G$1" pin="DEMP0" pad="24"/>
<connect gate="G$1" pin="DEMP1" pad="25"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="FMT0" pad="26"/>
<connect gate="G$1" pin="FMT1" pad="27"/>
<connect gate="G$1" pin="FMT2" pad="28"/>
<connect gate="G$1" pin="LRCK" pad="1"/>
<connect gate="G$1" pin="MUTE" pad="4"/>
<connect gate="G$1" pin="SCK" pad="5"/>
<connect gate="G$1" pin="VCCC" pad="15"/>
<connect gate="G$1" pin="VCCF" pad="21"/>
<connect gate="G$1" pin="VCCL" pad="20"/>
<connect gate="G$1" pin="VCCR" pad="10"/>
<connect gate="G$1" pin="VCOM" pad="14"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VOUTL+" pad="17"/>
<connect gate="G$1" pin="VOUTL-" pad="18"/>
<connect gate="G$1" pin="VOUTR+" pad="13"/>
<connect gate="G$1" pin="VOUTR-" pad="12"/>
<connect gate="G$1" pin="ZEROL" pad="23"/>
<connect gate="G$1" pin="ZEROR" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM1793DBR"/>
<attribute name="OC_FARNELL" value="1408322"/>
<attribute name="OC_NEWARK" value="61H5174"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BUF602" prefix="IC">
<description>&lt;b&gt;High-Speed, Closed-Loop Buffer&lt;/b&gt;&lt;p&gt;
Source: Burr-Brown buf602.pdf</description>
<gates>
<gate name="G$1" symbol="BUF602"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="8"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="5"/>
<connect gate="G$1" pin="VREF" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BUF602ID."/>
<attribute name="OC_FARNELL" value="1754777"/>
<attribute name="OC_NEWARK" value="34R6765"/>
</technology>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
<connect gate="G$1" pin="VREF" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BUF602IDBVT"/>
<attribute name="OC_FARNELL" value="1407166"/>
<attribute name="OC_NEWARK" value="67K7913"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RCV420" prefix="IC">
<description>&lt;b&gt;Precision 4mA to 20mA CURRENT LOOP RECEIVER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/rcv420.pdf</description>
<gates>
<gate name="G$1" symbol="RCV420"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="CT" pad="2"/>
<connect gate="G$1" pin="RCVCOM" pad="13"/>
<connect gate="G$1" pin="RCVFB" pad="15"/>
<connect gate="G$1" pin="RCVOUT" pad="14"/>
<connect gate="G$1" pin="REFCOM" pad="5"/>
<connect gate="G$1" pin="REFFB" pad="10"/>
<connect gate="G$1" pin="REFIN" pad="12"/>
<connect gate="G$1" pin="REFNOISE" pad="7"/>
<connect gate="G$1" pin="REFOUT" pad="11"/>
<connect gate="G$1" pin="REFTRIMM" pad="8"/>
<connect gate="G$1" pin="V+" pad="16"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="RCV420JP"/>
<attribute name="OC_FARNELL" value="1212342"/>
<attribute name="OC_NEWARK" value="60K6765"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7828" prefix="IC">
<description>&lt;b&gt;12-Bit, 8-Channel Sampling ANALOG-TO-DIGITAL CONVERTER with I2C? Interface&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. ADS7828.pdf</description>
<gates>
<gate name="G$1" symbol="ADS7828"/>
</gates>
<devices>
<device name="" package="TSSOP16-PW">
<connects>
<connect gate="G$1" pin="A0" pad="12"/>
<connect gate="G$1" pin="A1" pad="13"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="COM" pad="11"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="REFIN/REFOUT" pad="10"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VDD" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS7828E/250"/>
<attribute name="OC_FARNELL" value="1470338"/>
<attribute name="OC_NEWARK" value="74C7158"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA163" prefix="IC">
<description>&lt;b&gt;Low-Noise, Low-Distortion INSTRUMENTATION AMPLIFIER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ina163.pdf</description>
<gates>
<gate name="G$1" symbol="INA163"/>
</gates>
<devices>
<device name="" package="SO14">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="GS1" pad="3"/>
<connect gate="G$1" pin="GS2" pad="12"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="REF" pad="10"/>
<connect gate="G$1" pin="SENSE" pad="8"/>
<connect gate="G$1" pin="V+" pad="11"/>
<connect gate="G$1" pin="V-" pad="6"/>
<connect gate="G$1" pin="VO1" pad="1"/>
<connect gate="G$1" pin="VO2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="INA163UAE4"/>
<attribute name="OC_FARNELL" value="1206906"/>
<attribute name="OC_NEWARK" value="97K1930"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INA217" prefix="IC">
<description>&lt;b&gt;Low-Noise, Low-Distortion INSTRUMENTATION AMPLIFIER&lt;/b&gt; Replacement for SSM2017&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ina217.pdf</description>
<gates>
<gate name="G$1" symbol="INA217"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="5"/>
<connect gate="G$1" pin="RG1" pad="1"/>
<connect gate="G$1" pin="RG2" pad="8"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA217AIP"/>
<attribute name="OC_FARNELL" value="1212423"/>
<attribute name="OC_NEWARK" value="74C9859"/>
</technology>
</technologies>
</device>
<device name="DW" package="DW_RPDSO-G16">
<connects>
<connect gate="G$1" pin="+IN" pad="5"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="11"/>
<connect gate="G$1" pin="REF" pad="10"/>
<connect gate="G$1" pin="RG1" pad="2"/>
<connect gate="G$1" pin="RG2" pad="15"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="INA217AIDWT"/>
<attribute name="OC_FARNELL" value="1459470"/>
<attribute name="OC_NEWARK" value="02E2758"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PGA2500" prefix="IC">
<description>&lt;b&gt;Digitally Controlled Microphone Preamplifier&lt;/b&gt;&lt;p&gt;

Source: http://focus.ti.com/lit/ds/symlink/pga2500.pdf</description>
<gates>
<gate name="G$1" symbol="PGA2500"/>
</gates>
<devices>
<device name="DB" package="DB_R-PDSO-G28">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="!DCEN" pad="7"/>
<connect gate="G$1" pin="0DB" pad="8"/>
<connect gate="G$1" pin="AGND" pad="28"/>
<connect gate="G$1" pin="CS11" pad="24"/>
<connect gate="G$1" pin="CS12" pad="23"/>
<connect gate="G$1" pin="CS21" pad="22"/>
<connect gate="G$1" pin="CS22" pad="21"/>
<connect gate="G$1" pin="DGND" pad="6"/>
<connect gate="G$1" pin="GPO1" pad="1"/>
<connect gate="G$1" pin="GPO2" pad="2"/>
<connect gate="G$1" pin="GPO3" pad="3"/>
<connect gate="G$1" pin="GPO4" pad="4"/>
<connect gate="G$1" pin="OVR" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="12"/>
<connect gate="G$1" pin="SDI" pad="10"/>
<connect gate="G$1" pin="SDO" pad="13"/>
<connect gate="G$1" pin="VA+" pad="18"/>
<connect gate="G$1" pin="VA+@1" pad="19"/>
<connect gate="G$1" pin="VA-" pad="15"/>
<connect gate="G$1" pin="VA-@1" pad="20"/>
<connect gate="G$1" pin="VCOMIN" pad="25"/>
<connect gate="G$1" pin="VD-" pad="14"/>
<connect gate="G$1" pin="VIN+" pad="27"/>
<connect gate="G$1" pin="VIN-" pad="26"/>
<connect gate="G$1" pin="VOUT+" pad="17"/>
<connect gate="G$1" pin="VOUT-" pad="16"/>
<connect gate="G$1" pin="ZCEN" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
