<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.2">
<drawing>
<library>
<description>&lt;b&gt;Connector from KYCON, Inc&lt;/b&gt;&lt;p&gt;
1810 Little Orchard Street,&lt;br&gt;
San Jose,&lt;br&gt;
CA 95125 (408)494-0330&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/autor&gt;</description>
<packages>
<package name="KLDVX-0202-A">
<description>&lt;b&gt;Power Jack, Vertical, PCB Mount, 2.0 mm Center Pin&lt;/b&gt;&lt;p&gt;
Source: KLDVX-0202x.pdf</description>
</package>
<package name="KLDVX-0202-B">
<description>&lt;b&gt;Power Jack, Vertical, PCB Mount, 2.5 mm Center Pin&lt;/b&gt;&lt;p&gt;
Source: KLDVX-0202x.pdf</description>
</package>
<package name="KLDVX-0202-C">
<description>&lt;b&gt;Power Jack, Vertical, PCB Mount, 3.0 mm Center Pin&lt;/b&gt;&lt;p&gt;
Source: KLDVX-0202x.pdf</description>
</package>
<package name="GLX-S-88M">
<description>&lt;b&gt;Mod. Jack, Right Angle, 8 posiotion, 8 contatcs&lt;/b&gt; RJ45&lt;p&gt;
Source: GLX-S-88M.pdf</description>
</package>
<package name="KUSBVX">
<description>&lt;b&gt;Vertical,Top Entry Universal Serial Bus Connector&lt;/b&gt; KUSBVX Series&lt;p&gt;
Source: KYCON Sibalco USB vertical socket KUSBV.pdf</description>
</package>
<package name="KUSBVX-BS1N">
<description>&lt;b&gt;USB B-type Receptacle&lt;/b&gt; Vertical, 4 Position, Through Hole&lt;p&gt;
Source: Sibalco Kycon KUSBVX-BS1N-xxx.pdf</description>
</package>
</packages>
<symbols>
<symbol name="POWER-JACK_2-SWITCH">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1@1" direction="pas"/>
<pin name="3@1" direction="pas"/>
<pin name="2@1" direction="pas"/>
</symbol>
<symbol name="JACK8SH">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S1" direction="pas"/>
</symbol>
<symbol name="USB">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="S2" direction="pas"/>
<pin name="S1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="KLDVX-0202-">
<description>&lt;b&gt;Power Jack, Vertical, PCB Mount, 2.0 mm, 2.5 mm, 3.0 mm Center Pin&lt;/b&gt;&lt;p&gt;
Source: KLDVX-0202x.pdf</description>
<gates>
<gate name="G$1" symbol="POWER-JACK_2-SWITCH"/>
</gates>
<devices>
<device name="A" package="KLDVX-0202-A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="1@1" pad="1@1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="2@1" pad="2@1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3@1" pad="3@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="B" package="KLDVX-0202-B">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="1@1" pad="1@1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="2@1" pad="2@1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3@1" pad="3@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="C" package="KLDVX-0202-C">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="1@1" pad="1@1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="2@1" pad="2@1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="3@1" pad="3@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GLX-S-88M" prefix="X">
<description>&lt;b&gt;Mod. Jack, Right Angle, 8 posiotion, 8 contatcs&lt;/b&gt; RJ45&lt;p&gt;
Source: GLX-S-88M.pdf</description>
<gates>
<gate name="G$1" symbol="JACK8SH"/>
</gates>
<devices>
<device name="" package="GLX-S-88M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="S1" pad="S1"/>
<connect gate="G$1" pin="S2" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KUSBVX" prefix="X">
<description>&lt;b&gt;Vertical,Top Entry Universal Serial Bus Connector&lt;/b&gt; KUSBVX Series&lt;p&gt;
Source: KYCON Sibalco USB vertical socket KUSBV.pdf</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="" package="KUSBVX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="S1" pad="M1"/>
<connect gate="G$1" pin="S2" pad="M2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KUSBVX-BS1N" prefix="X">
<description>&lt;b&gt;USB B-type Receptacle&lt;/b&gt; Vertical, 4 Position, Through Hole&lt;p&gt;
Source: Sibalco Kycon KUSBVX-BS1N-xxx.pdf</description>
<gates>
<gate name="G$1" symbol="USB"/>
</gates>
<devices>
<device name="" package="KUSBVX-BS1N">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="S1" pad="M1"/>
<connect gate="G$1" pin="S2" pad="M2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
