<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Pulse Engineering, Inc.&lt;/b&gt;&lt;p&gt;
www.pulseeng.com
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="J1">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
</package>
<package name="JP">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
</package>
</packages>
<symbols>
<symbol name="J1006">
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="NC/4" direction="in"/>
<pin name="NC/5" direction="in"/>
</symbol>
<symbol name="J1026">
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="5" direction="in"/>
<pin name="4" direction="in"/>
</symbol>
<symbol name="J006-LED">
<pin name="C-R" direction="pas"/>
<pin name="A-R" direction="pas"/>
<pin name="C-L" direction="pas"/>
<pin name="A-L" direction="pas"/>
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="NC/4" direction="in"/>
<pin name="NC/5" direction="in"/>
</symbol>
<symbol name="J1012F21R">
<pin name="C-R" direction="pas"/>
<pin name="A-R" direction="pas"/>
<pin name="C-L" direction="pas"/>
<pin name="A-L" direction="pas"/>
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="8" direction="in"/>
</symbol>
<symbol name="J1011F">
<pin name="C-R" direction="pas"/>
<pin name="A-R" direction="pas"/>
<pin name="C-L" direction="pas"/>
<pin name="AL" direction="pas"/>
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="NC/4" direction="in"/>
<pin name="NC/5" direction="in"/>
</symbol>
<symbol name="J1026FX1">
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="5" direction="in"/>
<pin name="4" direction="in"/>
<pin name="C-R" direction="pas"/>
<pin name="A-R" direction="pas"/>
<pin name="C-L" direction="pas"/>
<pin name="A-L" direction="pas"/>
</symbol>
<symbol name="J1012F">
<pin name="C-R" direction="pas"/>
<pin name="A-R" direction="pas"/>
<pin name="C-L" direction="pas"/>
<pin name="A-L" direction="pas"/>
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="8" direction="in"/>
</symbol>
<symbol name="JP006">
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
</symbol>
<symbol name="JP011">
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="SH@1" direction="in"/>
<pin name="SH@2" direction="in"/>
<pin name="A-Y" direction="in"/>
<pin name="C-Y" direction="in"/>
<pin name="C-O_A-G" direction="in"/>
<pin name="A-O_C-G" direction="in"/>
</symbol>
<symbol name="JP026">
<pin name="TD+" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="TD-" direction="in"/>
<pin name="RD+" direction="in"/>
<pin name="CR" direction="in"/>
<pin name="RD-" direction="in"/>
<pin name="SH@2" direction="in"/>
<pin name="SH@1" direction="in"/>
<pin name="CY" direction="pas"/>
<pin name="AY" direction="pas"/>
<pin name="COG" direction="pas"/>
<pin name="AOG" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="J1006F01P" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="J006-LED"/>
</gates>
<devices>
<device name="" package="J1">
<connects>
<connect gate="G$1" pin="A-L" pad="12"/>
<connect gate="G$1" pin="A-R" pad="9"/>
<connect gate="G$1" pin="C-L" pad="11"/>
<connect gate="G$1" pin="C-R" pad="10"/>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="NC/4" pad="4"/>
<connect gate="G$1" pin="NC/5" pad="5"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="J1006F21" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="J1006"/>
</gates>
<devices>
<device name="" package="J1">
<connects>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="NC/4" pad="4"/>
<connect gate="G$1" pin="NC/5" pad="5"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="J1011F" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="J1011F"/>
</gates>
<devices>
<device name="" package="J1">
<connects>
<connect gate="G$1" pin="A-R" pad="9"/>
<connect gate="G$1" pin="AL" pad="12"/>
<connect gate="G$1" pin="C-L" pad="11"/>
<connect gate="G$1" pin="C-R" pad="10"/>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="NC/4" pad="4"/>
<connect gate="G$1" pin="NC/5" pad="5"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="01P">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="21P">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="J1012F21R" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="J1012F21R"/>
</gates>
<devices>
<device name="" package="J1">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A-L" pad="12"/>
<connect gate="G$1" pin="A-R" pad="10"/>
<connect gate="G$1" pin="C-L" pad="11"/>
<connect gate="G$1" pin="C-R" pad="9"/>
<connect gate="G$1" pin="CR" pad="5"/>
<connect gate="G$1" pin="CT" pad="2"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="J11012F" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="J1012F"/>
</gates>
<devices>
<device name="" package="J1">
<connects>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="A-L" pad="12"/>
<connect gate="G$1" pin="A-R" pad="10"/>
<connect gate="G$1" pin="C-L" pad="11"/>
<connect gate="G$1" pin="C-R" pad="9"/>
<connect gate="G$1" pin="CR" pad="5"/>
<connect gate="G$1" pin="CT" pad="2"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="6"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="01C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="21C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="21K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="J1026F01" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="J1026"/>
</gates>
<devices>
<device name="" package="J1">
<connects>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="J1026F" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="J1026FX1"/>
</gates>
<devices>
<device name="C" package="J1">
<connects>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A-L" pad="12"/>
<connect gate="G$1" pin="A-R" pad="10"/>
<connect gate="G$1" pin="C-L" pad="11"/>
<connect gate="G$1" pin="C-R" pad="9"/>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="21">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="J1">
<connects>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="A-L" pad="12"/>
<connect gate="G$1" pin="A-R" pad="9"/>
<connect gate="G$1" pin="C-L" pad="11"/>
<connect gate="G$1" pin="C-R" pad="10"/>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="RD+" pad="7"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="TD+" pad="1"/>
<connect gate="G$1" pin="TD-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JP006821U" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="JP006"/>
</gates>
<devices>
<device name="" package="JP">
<connects>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="1"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JP011821U" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="JP011"/>
</gates>
<devices>
<device name="" package="JP">
<connects>
<connect gate="G$1" pin="A-O_C-G" pad="9"/>
<connect gate="G$1" pin="A-Y" pad="8"/>
<connect gate="G$1" pin="C-O_A-G" pad="10"/>
<connect gate="G$1" pin="C-Y" pad="7"/>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="1"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SH@1" pad="SH1"/>
<connect gate="G$1" pin="SH@2" pad="SH2"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JP026851U" prefix="X">
<description>&lt;b&gt;PULSEJACK (TM) 1x1 Tab-UP RJ45&lt;/b&gt;&lt;p&gt;
10/100 Base-TX RJ45 1x1 Tab-UP with LEDs 8-pin (J1 series) and 6-pin (JP series) integrated magnetics connector,&lt;br&gt;
designed to support applications, such as ADSL modems, LAN-on-Motherboard, and Hub and Switches.&lt;br&gt;
Source: www.pulseeng.com .. PulseJack-J402.pdf</description>
<gates>
<gate name="G$1" symbol="JP026"/>
</gates>
<devices>
<device name="" package="JP">
<connects>
<connect gate="G$1" pin="AOG" pad="10"/>
<connect gate="G$1" pin="AY" pad="8"/>
<connect gate="G$1" pin="COG" pad="9"/>
<connect gate="G$1" pin="CR" pad="6"/>
<connect gate="G$1" pin="CT" pad="1"/>
<connect gate="G$1" pin="CY" pad="7"/>
<connect gate="G$1" pin="RD+" pad="4"/>
<connect gate="G$1" pin="RD-" pad="5"/>
<connect gate="G$1" pin="SH@1" pad="SH1"/>
<connect gate="G$1" pin="SH@2" pad="SH2"/>
<connect gate="G$1" pin="TD+" pad="2"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
