<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>&lt;BR&gt;&lt;big&gt;&lt;b&gt;GEYER ELECTRONIC --- Your producer for quartz crystals and oscillators&lt;/B&gt;&lt;/big&gt;&lt;br&gt;&lt;Hr&gt;

Version 1.0, 07.06.2016
&lt;hr&gt;
&lt;BR&gt;&lt;BR&gt; 

&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="320"&gt;&lt;/a&gt;&lt;p&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;GEYER ELECTRONIC e.K.&lt;/b&gt;&lt;br&gt;


Lochhamer Schlag 5&lt;br&gt;
D-82166 Gräfelfing/München&lt;br&gt;
&lt;br&gt;
Tel:   +49 89 546868-0&lt;br&gt;
Fax: +49 89 546868-90 für Batterien und Ladetechnik&lt;br&gt;
Fax: +49 89 546868-91 für Quarzprodukte&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.geyer-electronic.de"&gt;http://www.geyer-electronic.de&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:info@geyer-electronic.de"&gt;info@geyer-electronic.de&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor Geyer-Electronic does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

&lt;HR&gt;
Copyright: Geyer-Electronic</description>
<packages>
<package name="3.2X2.5_KX-7">
<description>4 Pad</description>
</package>
<package name="1.6X1.2">
<description>4 Pad</description>
</package>
<package name="2.0X1.6_KX-5">
<description>4 Pad</description>
</package>
<package name="2.5X2.0_KX-6">
<description>4 Pad</description>
</package>
<package name="5.0X3.2_KX-9A">
<description>4 Pad</description>
</package>
<package name="5.0X3.2_2">
<description>2 Pad</description>
</package>
<package name="6.0X3.5_4">
<description>4 Pad</description>
</package>
<package name="6.0X3.5_2">
<description>2 Pad</description>
</package>
<package name="7.0X5.0">
<description>4 Pad</description>
</package>
<package name="11.6X5.5">
<description>4 Pad</description>
</package>
<package name="11.4X4.5">
<description>2 Pad</description>
</package>
<package name="2.0X1.6_KXO-V94">
<description>4 Pad</description>
</package>
<package name="2.5X2.0_KXO-V95">
<description>4 Pad</description>
</package>
<package name="3.2X2.5_KXO-V96">
<description>4 Pad</description>
</package>
<package name="5.0X3.2_KXO-V99">
<description>4 Pad</description>
</package>
<package name="7.0X5.08_KXO-(V)97">
<description>4 Pad</description>
</package>
<package name="3.2X2.5_KXO-84-TCXO">
<description>4 Pad</description>
</package>
<package name="7.0X5.0_6">
<description>6 Pad</description>
</package>
<package name="2.0X1.6_KXO-81-TCXO">
<description>4 Pad</description>
</package>
<package name="2.5X2.0_KXO-86-TCXO">
<description>4 Pad</description>
</package>
<package name="5.0X3.2_KXO-83-TCXO">
<description>4 Pad</description>
</package>
<package name="7.0X5.0_KXO-82-VCTCXO">
<description>4 Pad</description>
</package>
<package name="2.0X1.6_KXO-81-VCTCXO">
<description>4 Pad</description>
</package>
<package name="2.5X2.0_KXO-86-VCTCXO">
<description>4 Pad</description>
</package>
<package name="3.2X2.5_KXO-84-VCTCXO">
<description>4 Pad</description>
</package>
<package name="5.0X3.2_KXO-83-VCTCXO">
<description>4 Pad</description>
</package>
<package name="7.0X5.0_KXO-82-TCXO">
<description>4 Pad</description>
</package>
<package name="1.25X1.05">
<description>2 Pad</description>
</package>
<package name="1.6X1.0">
<description>2 Pad</description>
</package>
<package name="2.0X1.2">
<description>2 Pad</description>
</package>
<package name="3.2X1.5">
<description>2 Pad</description>
</package>
<package name="8.2X3.8">
<description>4 Pad</description>
</package>
<package name="2.0X1.6_KXO-81">
<description>4 Pad</description>
</package>
<package name="7.0X5.0_KXO-82">
<description>4 Pad</description>
</package>
<package name="5.0X3.2_KXO-83">
<description>4 Pad</description>
</package>
<package name="2.5X2.0_KXO-86">
<description>4 Pad</description>
</package>
<package name="5.0X3.2_KXO-68">
<description>6 Pad</description>
</package>
<package name="7.0X5.0_KXO-67">
<description>6 Pad</description>
</package>
<package name="3.2X2.5_KXO-84">
<description>4 Pad</description>
</package>
<package name="5.0X3.2_KXO-V62">
<description>6 Pad</description>
</package>
<package name="7.0X5.0-KXO-V63">
<description>6 Pad</description>
</package>
<package name="5.0X3.2_KXO-V66">
<description>6 Pad</description>
</package>
<package name="7.0X5.0_KXO-V65">
<description>6 Pad</description>
</package>
<package name="5.0X3.2_KXO-56">
<description>4 Pad</description>
</package>
<package name="7.0X1.5">
<description>4 Pad</description>
</package>
</packages>
<symbols>
<symbol name="Q">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="QG">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="TS" direction="pas"/>
</symbol>
<symbol name="QVCXO-SINE">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="VC" direction="in"/>
</symbol>
<symbol name="QVCXO-CMOS_5">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="TS" direction="pas"/>
<pin name="VC" direction="in"/>
</symbol>
<symbol name="QVCXO-COMS_4">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="VC" direction="in"/>
</symbol>
<symbol name="QTCXO-SINE">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="TS/GND" direction="pas"/>
</symbol>
<symbol name="QTCXO-HCMOS">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="GND/NC" direction="pwr"/>
</symbol>
<symbol name="PECL">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="!OUT" direction="out"/>
<pin name="TRI" direction="in"/>
</symbol>
<symbol name="LVDS-VCXO">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="TS" direction="pas"/>
<pin name="VC" direction="in"/>
<pin name="!OUT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LVDS">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="TS" direction="pas"/>
<pin name="!OUT" direction="out"/>
<pin name="OUT" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="KX" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; Quartz Crystals (MHz) SMD:&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;KX - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
     
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Load&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Capacitance&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KX-4&lt;BR&gt;
      KX-5&lt;BR&gt;
      KX-6&lt;BR&gt;
      KX-7&lt;BR&gt;
      KX-9A&lt;BR&gt;
      KX-9B&lt;BR&gt;
      KX-12A&lt;BR&gt;
      KX-12B&lt;BR&gt;
      KX-13&lt;BR&gt;
      KX-20&lt;BR&gt;
      KX-K&lt;BR&gt;
      KX-KS&lt;BR&gt; &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      1.6/1.2/0.3&lt;BR&gt;
      2.0/1.6/0.45&lt;BR&gt;
      2.5/2.0/0.55&lt;BR&gt;
      3.2/2.5/0.8&lt;BR&gt;
      5.0/3.2/1.0 &lt;BR&gt;
      5.0/3.2/1.1 &lt;BR&gt;
      6.0/3.5/1.1 &lt;BR&gt;
      6.0/3.5/1.0 &lt;BR&gt;
      7.0/5.0 /1.3 &lt;BR&gt;
      11.6/5.5/1.6 &lt;BR&gt;
      12.3/4.5/4.2 &lt;BR&gt;
      12.3/4.5/3.2 &lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      24.0 ~ 80.0 MHz&lt;BR&gt;
      16.0 ~ 80.0 MHz&lt;BR&gt;
      12.0 ~ 80.0 MHz&lt;BR&gt;
      8.0 ~ 60.0 MHz&lt;BR&gt;
      7,68 ~ 300,0 MHz&lt;BR&gt;
      8,0 ~ 50,0 MHz&lt;BR&gt;
      8,0 ~ 150,0 MHz&lt;BR&gt;
      8,0 ~ 50,0 MHz&lt;BR&gt;
      6,0 ~ 160,0 MHz&lt;BR&gt;
      3,579 ~ 25,0 MHz&lt;BR&gt;
      3,579 ~ 70,0 MHz&lt;BR&gt;
      3,579 ~ 70,0 MHz&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     (*) -40°C …+85°C&lt;BR&gt;
     (*) -40°C …+125°C&lt;BR&gt;
     (*) -40°C …+125°C&lt;BR&gt;     
     (*) -40°C …+125°C&lt;BR&gt;
     (*) -40°C …+105°C&lt;BR&gt;
     (*) -40°C …+105°C&lt;BR&gt;
     (*) -40°C …+125°C&lt;BR&gt;
     (*) -40°C …+105°C&lt;BR&gt;
     (*) -40°C …+105°C&lt;BR&gt;
     (*) -40°C …+105°C&lt;BR&gt;
     (*) -40°C …+85°C&lt;BR&gt;
     (*) -40°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      8, 8…16&lt;BR&gt;
      8, 8…16&lt;BR&gt;
      10, 8…16&lt;BR&gt;
      12, 7…20&lt;BR&gt;
      16, 10…20&lt;BR&gt;
      16, 10…20&lt;BR&gt;
      16, 10…20&lt;BR&gt;
      16, 12…20&lt;BR&gt;
      16, 12…20&lt;BR&gt;
      16, 12…20&lt;BR&gt;
      16, 12…30&lt;BR&gt;
      16, 12…30&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
     yes&lt;BR&gt;
      yes&lt;BR&gt;
    yes&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-4.pdf"&gt;KX-4.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-5.pdf"&gt;KX-5.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-6.pdf"&gt;KX-6.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-7.pdf"&gt;KX-7.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-9A.pdf"&gt;KX-9A.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-9B.pdf"&gt;KX-9B.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-12A.pdf"&gt;KX-12A.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-12B.pdf"&gt;KX-12B.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-13.pdf"&gt;KX-13.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-20.pdf"&gt;KX-20.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-K.pdf"&gt;KX-K.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-KS.pdf"&gt;KX-KS.pdf&lt;/a&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KX4,KX5,KX6,KX7,KX9A,KX9B,KX12A,KX12B,KX13,KX20,KXK,KXKS;1612;2016;2520;3225;5032;6035;7050;11655;12345;1,6x1,2;2,0x1,6;2,5x2,0;3,2x2,5;5,0x3,2;6,0x3,5;7,0x5,0;11,6x5,5;12,3x4,5;12,3x4,5;1.6x1.2;2.0x1.6;2.5x2.0;3.2x2.5;5.0x3.2;6.0x3.5;7.0x5.0;11.6x5.5;12.3x4.5;12.3x4.5;&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="-7" package="3.2X2.5_KX-7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-4" package="1.6X1.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-5" package="2.0X1.6_KX-5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-6" package="2.5X2.0_KX-6">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-9A" package="5.0X3.2_KX-9A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-9B" package="5.0X3.2_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-12A" package="6.0X3.5_4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-12B" package="6.0X3.5_2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-13" package="7.0X5.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-20" package="11.6X5.5">
<connects>
<connect gate="G$1" pin="1" pad="1 4"/>
<connect gate="G$1" pin="2" pad="2 3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-K" package="11.4X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-KS" package="11.4X4.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KX-327" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; Tuning Fork Crystals (kHz) SMD:&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;KX327 - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Load&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Capacitance&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KX-327VT&lt;BR&gt;
      KX-327FT&lt;BR&gt;
      KX-327RT&lt;BR&gt;
      KX-327NHT&lt;BR&gt;
      KX-327NHF&lt;BR&gt;
      KX-327L&lt;BR&gt;
      KX-327S&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      1.25/1.05/0.5&lt;BR&gt;
      1.6/1.0/0.5&lt;BR&gt;
      2.0/1.2/0.6&lt;BR&gt;
      3.2/1.5/0.8&lt;BR&gt;
      3.2/1.5/0.8&lt;BR&gt;
      7.0/1.5/1.4&lt;BR&gt;
      8.2/3.8/2.5&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      32,768 kHz&lt;BR&gt;
      32,768 kHz&lt;BR&gt;
      32,768 kHz&lt;BR&gt;
      32,768 kHz&lt;BR&gt;
      32,768 kHz&lt;BR&gt;
      32,768 kHz&lt;BR&gt;
      32,768 kHz&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±10 … ±20ppm&lt;BR&gt;
      ±10 … ±20ppm&lt;BR&gt;
      ±10 … ±20ppm&lt;BR&gt;
      ±10 … ±20ppm&lt;BR&gt;
      ±10 … ±20ppm&lt;BR&gt;
      ±10 … ±20ppm&lt;BR&gt;
      ±5 … ±20ppm&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
(*) -40°C …+85°C&lt;BR&gt;
(*) -40°C …+85°C&lt;BR&gt;
(*) -40°C …+85°C&lt;BR&gt;
(*) -40°C …+85°C&lt;BR&gt;
(*) -40°C …+125°C&lt;BR&gt;
(*) -40°C …+85°C&lt;BR&gt;
(*) -40°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       7/9/12,5&lt;BR&gt;
       7/9/12,5&lt;BR&gt;
       7/9/12,6&lt;BR&gt;
       7/9/12,5&lt;BR&gt;
       9/12,5&lt;BR&gt;
       7/9/12,5&lt;BR&gt;
       6/12,5&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      yes&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-327VT.pdf"&gt;KX-327VT.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-327FT.pdf"&gt;KX-327FT.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-327RT.pdf"&gt;KX-327RT.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-327NHT.pdf"&gt;KX-327NHT.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-327NHF.pdf"&gt;KX-327NHF.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-327L.pdf"&gt;KX-327L.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KX-327S.pdf"&gt;KX-327S.pdf&lt;/a&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KX327VT,KX327FT,KX327RT,KX327NHT,KX327NHF,KX327S,KX327L;125105;1610;2012;3215;7015;8238;1,25x1,05,1.25x1.05;1,6x1,0,1.6x1.0;2,0x1,2,2.0x1.2;3,2x1,5,3.2x1.5;8,2x3,8,8.2x3.8,7.0x1.5,7,0x1,532.768kHz&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="Q"/>
</gates>
<devices>
<device name="-VT" package="1.25X1.05">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FT" package="1.6X1.0">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RT" package="2.0X1.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-NHT" package="3.2X1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-NHF" package="3.2X1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-S" package="8.2X3.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-L" package="7.0X1.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-PXO/XO-V" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; Clock Oscillator (PXO/XO) MHz :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;KXO-V - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-V94&lt;BR&gt;
      KXO-V94&lt;BR&gt;
      KXO-V95&lt;BR&gt;
      KXO-V95&lt;BR&gt;
      KXO-V96&lt;BR&gt;
      KXO-V96&lt;BR&gt;
      KXO-V99&lt;BR&gt;
      KXO-V99&lt;BR&gt;
      KXO-97&lt;BR&gt;
      KXO-V97&lt;BR&gt;
      KXO-97 - KXO-V97&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      2.0/1.6/0.80&lt;BR&gt;
      2.0/1.6/0.80&lt;BR&gt;
      2.5/2.0/0.82&lt;BR&gt; 
      2.5/2.0/0.82&lt;BR&gt; 
      3.2/2.5/1.2 &lt;BR&gt;
      3.2/2.5/1.2 &lt;BR&gt;
      5.0/3.2/1.2 &lt;BR&gt;
      5.0/3.2/1.2 &lt;BR&gt;
      7.0/5.08/1.3&lt;BR&gt;
      7.0/5.08/1.3&lt;BR&gt;
      7.0/5.08/1.3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       32,768 kHz&lt;BR&gt;
       1,0 ~ 80,0 MHz&lt;BR&gt;
       32,768 kHz&lt;BR&gt;
       1,0 ~ 70,0 MHz&lt;BR&gt;
       32,768 kHz&lt;BR&gt;
       1,0 ~ 156,0 MHz&lt;BR&gt;
       32,768 kHz&lt;BR&gt;
       1,0 ~ 200,0 MHz&lt;BR&gt;
       32,768 kHz&lt;BR&gt;
       32,768 kHz&lt;BR&gt;
       1,0 ~ 160,0 MHz&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;

&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;
       HCMOS&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
     -&lt;BR&gt;
      yes&lt;BR&gt;
      yes&lt;BR&gt;
      yes&lt;BR&gt;
      yes&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V94-kHz.pdf"&gt;KXO-V94-kHz.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V94.pdf"&gt;KXO-V94.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V95-kHz.pdf"&gt;KXO-V95-kHz.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V95.pdf"&gt;KXO-V95.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V96-kHz.pdf"&gt;KXO-V96-kHz.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V96.pdf"&gt;KXO-V96.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V99-kHz.pdf"&gt;KXO-V99-kHz.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V99.pdf"&gt;KXO-V99.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-97-kHz.pdf"&gt;KXO-97-kHz.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V97-kHz.pdf"&gt;KXO-V97-kHz.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V97.pdf"&gt;KXO-V97.pdf&lt;/a&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#aaaaaa" size="1"&gt;&amp;nbsp;Hans Locher&lt;/font&gt;&lt;/b&gt;
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXOV94,KXOV95;KXOV96;KXOV97;KXO97;2016;2520;3225;5032;70508;2,5x2,0;3,2x2,5;5,0x3,2;7,0x5,08;2.5x2.0;3.2x2.5;5.0x3.2;7.0x5.08;&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QG"/>
</gates>
<devices>
<device name="94" package="2.0X1.6_KXO-V94">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="95" package="2.5X2.0_KXO-V95">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="96" package="3.2X2.5_KXO-V96">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="99" package="5.0X3.2_KXO-V99">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="97" package="7.0X5.08_KXO-(V)97">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-PXO/XO-56" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; SSO Spread Spectrum Oscillator (PXO/XO) MHz :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;KXO - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-56&lt;BR&gt;
      &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      5.0/3.2/1.2 &lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       1,0 ~ 134,0 MHz&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±25 … ±100ppm&lt;BR&gt;
    &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       HCMOS&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
  &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-56.pdf"&gt;KXO-56.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXO56;5,0x3,2;5.0x3.2;5032&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QG"/>
</gates>
<devices>
<device name="-56" package="5.0X3.2_KXO-56">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-VCXO-SINE" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; VCXO :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;Sinewave - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-81&lt;BR&gt;
      KXO-86&lt;BR&gt;
      KXO-84&lt;BR&gt;
      KXO-83&lt;BR&gt;
      KXO-82&lt;BR&gt;
      &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      2.0/1.6/0.7&lt;BR&gt;
      2.5/2.0/0.7&lt;BR&gt; 
      3.2/2.5/1.0 &lt;BR&gt;
      5.0/3.2/1.5 &lt;BR&gt;
      7.0/5.0/2.0&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       13,0 ~ 40,0 MHz&lt;BR&gt;
       13,0 ~ 40,0 MHz&lt;BR&gt;
       10,0 ~ 26,0 MHz&lt;BR&gt;
       12,0 ~ 26,0 MHz&lt;BR&gt;
       12,6 ~ 20,0 MHz&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      (*) -30°C …+75°C&lt;BR&gt;
      (*) -30°C …+75°C&lt;BR&gt;
      (*) -40°C …+85°C&lt;BR&gt;
      (*) -40°C …+85°C&lt;BR&gt; 
      (*) -30°C …+80°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
     -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-81-VCXO-sinewave.pdf"&gt;KXO-81.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-86-VCXO-sinewave.pdf"&gt;KXO-86.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-84-VCXO-sinewave.pdf"&gt;KXO-84.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-83-VCXO-sinewave.pdf"&gt;KXO-83.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-82-VCXO-sinewave.pdf"&gt;KXO-82.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXO81,KXO86,KXO84,KXO83,KXO82,2,0x1,6;2.0x1.6;2,5x2,0;2.5x2.0;3,2x2,5;3.2x2.5;5,0x3,2;5.0x3.2;7,0x5,0;7.0x5.0;2016;2520;3225;5032;7050&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QVCXO-SINE"/>
</gates>
<devices>
<device name="-81" package="2.0X1.6_KXO-81">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-86" package="2.5X2.0_KXO-86">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-83" package="5.0X3.2_KXO-83">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-82" package="7.0X5.0_KXO-82">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-84" package="3.2X2.5_KXO-84">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-VCXO-CMOS_5" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; VCXO :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;CMOS - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-75&lt;BR&gt;
      KXO-75R&lt;BR&gt;
          &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      7.0/5.0/1.7&lt;BR&gt;
      7.0/5.0/1.7&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       1,544 ~ 77,760 MHz&lt;BR&gt;
       1,544 ~ 77,760 MHz&lt;BR&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±10 … ±50ppm&lt;BR&gt;
      ±10 … ±50ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -10°C …+85°C&lt;BR&gt;
       (*) -10°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       CMOS&lt;BR&gt;
       CMOS&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
     -&lt;BR&gt;
 &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-75.pdf"&gt;KXO-75.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-75R.pdf"&gt;KXO-75R.pdf&lt;/a&gt;&lt;BR&gt;

&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXO75,KXO75R,7,0x5,0;7.0x5.0;7050&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QVCXO-CMOS_5"/>
</gates>
<devices>
<device name="75" package="7.0X5.0_6">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="TS" pad="5"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="75R" package="7.0X5.0_6">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="TS" pad="2"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-VCXO-CMOS_4" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; VCXO :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;CMOS - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-84&lt;BR&gt;
          &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      3.2/2.5/1.0&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       1.25 ~ 54.0 MHz&lt;BR&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±10 … ±50ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       CMOS&lt;BR&gt;

&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
 &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-84-VCXO-CMOS.pdf"&gt;KXO-84.pdf&lt;/a&gt;&lt;BR&gt;

&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KX84;3,2x2,5;3.2x2.5;3225&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QVCXO-COMS_4"/>
</gates>
<devices>
<device name="" package="3.2X2.5_KXO-84-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-TCXO-SINE" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; TCXO :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;Sinewave - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-81&lt;BR&gt;
      KXO-86&lt;BR&gt;
      KXO-84&lt;BR&gt;
      KXO-83&lt;BR&gt;
      KXO-82&lt;BR&gt;
      &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      2.0/1.6/0.7&lt;BR&gt;
      2.5/2.0/0.7&lt;BR&gt; 
      3.2/2.5/1.0 &lt;BR&gt;
      5.0/3.2/1.5 &lt;BR&gt;
      7.0/5.0/2.0&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       13,0 ~ 52,0 MHz&lt;BR&gt;
       12,0 ~ 26,0 MHz&lt;BR&gt;
       10,0 ~ 40,0 MHz&lt;BR&gt;
       12,0 ~ 26,0 MHz&lt;BR&gt;
       12,6 ~ 20,0 MHz&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -30°C …+75°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -30°C …+80°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
     -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-81-TCXO-sinewave.pdf"&gt;KXO-81.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-86-TCXO-sinewave.pdf"&gt;KXO-86.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-84-TCXO-sinewave.pdf"&gt;KXO-84.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-83-TCXO-sinewave.pdf"&gt;KXO-83.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-82-TCXO-sinewave.pdf"&gt;KXO-82.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXO81,KXO86,KXO84,KXO83,KXO82;2016;2520;3225;5032;7050;2,0x1,6;2,5x2,0;3,2x2,5;5,0x3,2;7,0x5,0;2,0x1,6;2.5x2.0;3.2x2.5;5.0x3.2;7.0x5.0;&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QTCXO-SINE"/>
</gates>
<devices>
<device name="-81" package="2.0X1.6_KXO-81-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS/GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-86" package="2.5X2.0_KXO-86-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS/GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-84" package="3.2X2.5_KXO-84-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS/GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-83" package="5.0X3.2_KXO-83-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS/GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-82" package="7.0X5.0_KXO-82-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TS/GND" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-TCXO-CMOS" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; TCXO :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;CMOS - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-86&lt;BR&gt;
      KXO-84&lt;BR&gt;
      KXO-83&lt;BR&gt;
      KXO-82&lt;BR&gt;
      &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      2.5/2.0/0.7&lt;BR&gt; 
      3.2/2.5/1.0 &lt;BR&gt;
      5.0/3.2/1.5&lt;BR&gt; 
      7.0/5.0/2.4 &lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       13,0 ~ 40,0 MHz&lt;BR&gt;
       10,0 ~ 40,0 MHz&lt;BR&gt;
       10,0 ~ 40,0 MHz&lt;BR&gt;
       10,0 ~ 30,0 MHz&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±3,0ppm&lt;BR&gt;
      ±1,0 … ±3,0ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -30°C …+75°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -30°C …+80°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       CMOS&lt;BR&gt;
       CMOS&lt;BR&gt;
       CMOS&lt;BR&gt;
       CMOS&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-86-TCXO-HCMOS.pdf"&gt;KXO-86.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-84-TCXO-HCMOS.pdf"&gt;KXO-84.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-83-TCXO-HCMOS.pdf"&gt;KXO-83.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-82-TCXO-HCMOS.pdf"&gt;KXO-82.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXO86,KXO84,KXO83,KXO82;2550;3225;5032;7050;2,5x2,0;3,2x2,5;2.5x2.0;3.2x2.5,5,0x3,2;7,0x5,0,5.0x3.2,7.0x5.0&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QTCXO-HCMOS"/>
</gates>
<devices>
<device name="-86" package="2.5X2.0_KXO-86-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND/NC" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-84" package="3.2X2.5_KXO-84-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND/NC" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-83" package="5.0X3.2_KXO-83-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND/NC" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-82" package="7.0X5.0_KXO-82-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND/NC" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-VCTCXO-SINE" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; VCTCXO :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;Sinewave - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;

    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-81&lt;BR&gt;
      KXO-86&lt;BR&gt;
      KXO-84&lt;BR&gt;
      KXO-83&lt;BR&gt;
      KXO-82&lt;BR&gt;
      &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      2.0/1.6/0.7&lt;BR&gt;
      2.5/2.0/0.7&lt;BR&gt; 
      3.2/2.5/1.0 &lt;BR&gt;
      5.0/3.2/1.5 &lt;BR&gt;
      7.0/5.0/2.0&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       13,0 ~ 40,0 MHz&lt;BR&gt;
       13,0 ~ 40,0 MHz&lt;BR&gt;
       8,0 ~ 40,0 MHz&lt;BR&gt;
       12,0 ~ 26,0 MHz&lt;BR&gt;
       12,6 ~ 20,0 MHz&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
      ±1,0 … ±2,5ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -30°C …+75°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -30°C …+80°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
       Sinewave&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
     -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-81-VCTCXO-sinewave.pdf"&gt;KXO-81.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-86-VCTCXO-sinewave.pdf"&gt;KXO-86.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-84-VCTCXO-sinewave.pdf"&gt;KXO-84.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-83-VCTCXO-sinewave.pdf"&gt;KXO-83.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-82-VCTCXO-sinewave.pdf"&gt;KXO-82.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXO81,KXO86,KXO84,KXO83,KXO82,2016;2520;3225;5032;7050;2,0x1,6;2,5x2,0;3,2x2,5;5,0x3,2;7,0x5,0;2.0x1.6;2.5x2.0;3.2x2.5;5.0x3.2;7.0x5.0;&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QVCXO-SINE"/>
</gates>
<devices>
<device name="-81" package="2.0X1.6_KXO-81-VCTCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-86" package="2.5X2.0_KXO-86-VCTCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-84" package="3.2X2.5_KXO-84-VCTCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-83" package="5.0X3.2_KXO-83-VCTCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-82" package="7.0X5.0_KXO-82-VCTCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-VCTCXO-CMOS" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; VCTCXO :&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;HCMOS - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;

    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Output&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-84&lt;BR&gt;
      &lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      3.2/2.5/1.0 &lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       8,0 ~ 40,0 MHz&lt;BR&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;      
      ±1,0 … ±2,5ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
        HCMOS&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-84-VCTCXO-HCMOS.pdf"&gt;KXO-84.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXO84;3,2x2,5;3.2x2.5;3225&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="QVCXO-COMS_4"/>
</gates>
<devices>
<device name="-84" package="3.2X2.5_KXO-84-VCTCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-PECL" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; Positiv Emitter Coupled Oszillator:&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;PECL - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Load&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Capacitance&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-68&lt;BR&gt;
      KXO-67&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      5.0/3.2/1.2&lt;BR&gt;
      7.0/5.0/1.7&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25,0 - 180,0&lt;BR&gt;
      50,0 - 252,5&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
      -&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-68.pdf"&gt;KXO-68.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-67.pdf"&gt;KXO-67.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXO86,KXO67,5,0x3,2,5.0x3.2,7.0x5.0,7,0x5,0;5032;7050&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PECL"/>
</gates>
<devices>
<device name="-68" package="5.0X3.2_KXO-68">
<connects>
<connect gate="G$1" pin="!OUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="TRI" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-67" package="7.0X5.0_KXO-67">
<connects>
<connect gate="G$1" pin="!OUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="TRI" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-LVDS-VCXO" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; LVDS-VCXO:&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;KXO-V6x - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Load&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Capacitance&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-V62&lt;BR&gt;
      KXO-V63&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      5.0/3.2/1.2&lt;BR&gt;
      7.0/5.0/1.7&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      20,0 - 700,0&lt;BR&gt;
      20,0 - 700,5&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
      -&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V62.pdf"&gt;KXO-V62.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V63.pdf"&gt;KXO-V63.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXOV62,KXOV63,5,0x3,2,5.0x3.2,7.0x5.0,7,0x5,0;5032;7050&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LVDS-VCXO"/>
</gates>
<devices>
<device name="-V63" package="7.0X5.0-KXO-V63">
<connects>
<connect gate="G$1" pin="!OUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="TS" pad="2"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-V62" package="5.0X3.2_KXO-V62">
<connects>
<connect gate="G$1" pin="!OUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="TS" pad="2"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KXO-LVDS" prefix="Q" uservalue="yes">
<description>&lt;P&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="80%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;th&gt;
&lt;b&gt;&lt;big&gt; LVDS Clock Oscillator:&lt;/big&gt;&lt;/B&gt;
&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;&amp;nbsp;KXO-V6x - Serie&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;/th&gt;
&lt;TABLE BORDER=1 CELLSPACING=2 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Model&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Size&amp;nbsp;l/w/h&amp;nbsp;[mm]&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&amp;nbsp;Range&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Frequency&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Stability&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Temp.&amp;nbsp;Range&amp;nbsp;[°C]&lt;/B&gt;&lt;/FONT&gt;

    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Load&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Capacitance&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AECQ 200&lt;br&gt;&lt;/B&gt;&lt;/FONT&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;availabel&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;Datasheet&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      KXO-V66&lt;BR&gt;
      KXO-V65&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;    
      5.0/3.2/1.2&lt;BR&gt;
      7.0/5.0/1.7&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      40,0 - 600,0 MHz&lt;BR&gt;
      19,440 - 700,0 MHz&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ±25 … ±100ppm&lt;BR&gt;
      ±25 … ±100ppm&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
       (*) -40°C …+85°C&lt;BR&gt;
       (*) -40°C …+85°C&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
     -&lt;BR&gt;
      -&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V66.pdf"&gt;KXO-V66.pdf&lt;/a&gt;&lt;BR&gt;
      &lt;a href="http://www.geyer-electronic.de/uploads/tx_userartikelfrequenz/GEYER-KXO-V65.pdf"&gt;KXO-V65.pdf&lt;/a&gt;&lt;BR&gt;
&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;

&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;


&lt;P&gt;
&lt;br&gt;&lt;a href="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" title="Enlarge picture"&gt;
&lt;img src="http://www.geyer-electronic.de/fileadmin/template/img/logo-geyer-electronic.png" width="150"&gt;&lt;/a&gt;&lt;p&gt;

Details see: &lt;a href="http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html"&gt;http://www.geyer-electronic.de/Frequenz-Produkte.9.0.html&lt;/a&gt;&lt;p&gt;

Created 2016-06-07, Hans Locher&lt;br&gt;
2016 (C) Geyer Quartz Technology
&lt;br&gt;
&lt;b&gt;&lt;font color="#ffffff" size="1"&gt;&amp;nbsp;KXOV66,KXOV65,5,0x3,2,5.0x3.2,7.0x5.0,7,0x5,0;5032;7050&lt;/font&gt;&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LVDS"/>
</gates>
<devices>
<device name="-V66" package="5.0X3.2_KXO-V66">
<connects>
<connect gate="G$1" pin="!OUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-V65" package="7.0X5.0_KXO-V65">
<connects>
<connect gate="G$1" pin="!OUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="TS" pad="1"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
