<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.1">
<drawing>
<library>
<description>&lt;b&gt;Microcontroller with USB Port&lt;/b&gt;&lt;p&gt;
Based on Cypress-EZ-usb-8051.pdf</description>
<packages>
<package name="PQFP80">
<description>&lt;b&gt;Plastic Quad Flat Package&lt;/b&gt;&lt;p&gt;
from micro-philips.lbr</description>
</package>
<package name="TQFP48_7X7">
<description>&lt;b&gt;Thin Quad Flat Package&lt;/b&gt;&lt;p&gt;
from SMD-IPC.lbr SQFP48 7x7</description>
</package>
<package name="PQFP44">
<description>&lt;b&gt;Plastic Quad Flat Package&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="LOGO">
<description>Cypress logo</description>
</package>
<package name="QFN48">
<description>&lt;b&gt;48-pin QFN 7 x 7 mm LF48&lt;/b&gt;&lt;p&gt;
48 Quad Flat Package No Leads&lt;br&gt;
Source: http://v4.cypress.com/cfuploads/img/products/cywusb6934.pdf</description>
</package>
<package name="SOIC28-EPAD">
<description>&lt;b&gt;28-pin (300-Mil) SOIC EPAD SE28.3&lt;/b&gt;&lt;p&gt;
Source: http://v4.cypress.com/cfuploads/img/products/cywusb6934.pdf</description>
</package>
<package name="SQFP-R-14X20-128">
<description>&lt;b&gt;QFP128&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, rectangle</description>
</package>
<package name="SQFP-R-14X20-100">
<description>&lt;b&gt;QFP100&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, rectangle</description>
</package>
<package name="SSOP56">
<description>&lt;b&gt;56-lead Shrunk Small Outline Package O56&lt;/b&gt;&lt;p&gt;
Source: Source: http://www.cypress.com .. cy7c68013a_5.pdf</description>
</package>
<package name="QFN56">
<description>&lt;b&gt;56-Lead QFN 8 x 8 mm LF56A&lt;/b&gt;&lt;p&gt;
Source: Source: http://www.cypress.com .. cy7c68013a_5.pdf</description>
</package>
<package name="VFBGA56">
<description>&lt;b&gt;VFBGA 56&lt;/b&gt;&lt;p&gt;
Source: Source: http://www.cypress.com .. cy7c68013a_5.pdf</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO20L">
<description>&lt;b&gt;20-Lead (300-MIL) SOIC S5&lt;/b&gt;&lt;p&gt;
Source: www.cypress.com .. CY7C6301XX.pdf</description>
</package>
<package name="SO24L">
<description>&lt;b&gt;24-Lead (300-Mil) SOIC S13&lt;/b&gt;&lt;p&gt;
Source: www.cypress.com .. CY7C6301XX.pdf</description>
</package>
<package name="QSOP24">
<description>&lt;b&gt;24-Lead Quarter Size Outline Q13&lt;/b&gt;&lt;p&gt;
Source: www.cypress.com .. CY7C6301XX.pdf</description>
</package>
<package name="SOIC28-3">
<description>&lt;b&gt;28-Pin SOIC&lt;/b&gt; Body 7.63 mm&lt;p&gt;
Source: http://www.cypress.com .. CY8C21345.pdf</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;44-Pin TQFP&lt;/b&gt;&lt;p&gt;
Source: http://www.cypress.com .. CY8C213452.pdf</description>
</package>
<package name="SOIC16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
16-Pin (150-Mil) SOIC&lt;br&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;
20-Pin (210-MIL) SSOP&lt;br&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
</package>
<package name="SSOP28">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;
28-Pin (210-MIL) SSOP&lt;br&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
</package>
<package name="QFN32-MAX06">
<description>&lt;b&gt;32-Pin (5x5 mm 0.60 MAX) QFN&lt;/b&gt;&lt;p&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
</package>
<package name="QFN32-SAWN">
<description>&lt;b&gt;32-Pin (5x5 mm Sawn) QFN&lt;/b&gt;&lt;p&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
</package>
<package name="QFN32">
<description>&lt;b&gt;32-Pin (5x5 mm) QFN&lt;/b&gt;&lt;p&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
</package>
<package name="TQFP100-14X14">
<description>&lt;b&gt;TQFP100&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;</description>
</package>
</packages>
<symbols>
<symbol name="EZ-USB-2131Q">
<pin name="XOUT" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="EA" direction="in"/>
<pin name="A0" direction="out"/>
<pin name="PSEN" direction="out"/>
<pin name="SCL" direction="oc"/>
<pin name="SDA" direction="oc"/>
<pin name="PA1/T1OUT"/>
<pin name="RESET" direction="in"/>
<pin name="PA3/!CS"/>
<pin name="PA4/!FRW"/>
<pin name="PA5/!FRD"/>
<pin name="PA6/RXD0OUT"/>
<pin name="PA7/RXD1OUT"/>
<pin name="PB0/T2"/>
<pin name="PB1/T2EX"/>
<pin name="PB2/RXD1"/>
<pin name="PB3/TXD1"/>
<pin name="PB4/INT4"/>
<pin name="PB5/!INT5"/>
<pin name="PA2/!OE"/>
<pin name="PA0/T0OUT"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="!DISCON" direction="out"/>
<pin name="USBD+" direction="hiz"/>
<pin name="USBD-" direction="hiz"/>
<pin name="BKPT" direction="out"/>
<pin name="PB6/INT6"/>
<pin name="PB7/T2OUT"/>
<pin name="PC0/RXD0"/>
<pin name="PC1/TXD0"/>
<pin name="PC2/!INT0"/>
<pin name="PC3/!INT1"/>
<pin name="PC4/T0"/>
<pin name="PC5/T1"/>
<pin name="PC6/!WR"/>
<pin name="PC7/!RD"/>
<pin name="CLK24" direction="out"/>
<pin name="!WAKEUP" direction="in"/>
<pin name="VCC3.3@1" direction="pwr"/>
<pin name="VCC3.3@2" direction="pwr"/>
<pin name="VCC3.3@3" direction="pwr"/>
<pin name="VCC3.3@4" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND/TEST" direction="pwr"/>
<pin name="GND/TEST1" direction="pwr"/>
<pin name="GND/TEST2" direction="pwr"/>
<pin name="GND/TEST3" direction="pwr"/>
<pin name="GND/TEST4" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
</symbol>
<symbol name="EZ-USB-2126T">
<pin name="XOUT" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="SCL" direction="oc"/>
<pin name="SDA" direction="oc"/>
<pin name="RESET" direction="in"/>
<pin name="PA6/RXD0OUT"/>
<pin name="PA7/RXD1OUT"/>
<pin name="PA0/T0OUT"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="!DISCON" direction="out"/>
<pin name="USBD+" direction="hiz"/>
<pin name="USBD-" direction="hiz"/>
<pin name="BKPT" direction="out"/>
<pin name="PC0/RXD0"/>
<pin name="PC1/TXD0"/>
<pin name="PC2/!INT0"/>
<pin name="PC3/!INT1"/>
<pin name="PC4/T0"/>
<pin name="PC5/T1"/>
<pin name="PC6/!WR"/>
<pin name="PC7/!RD"/>
<pin name="CLK24" direction="out"/>
<pin name="!WAKEUP" direction="in"/>
<pin name="CPU12MHZ" direction="in"/>
<pin name="VCC3.3@1" direction="pwr"/>
<pin name="VCC3.3@2" direction="pwr"/>
<pin name="VCC3.3@3" direction="pwr"/>
<pin name="VCC3.3@4" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND/TEST" direction="pwr"/>
<pin name="GND/TEST1" direction="pwr"/>
<pin name="GND/TEST2" direction="pwr"/>
<pin name="GND/TEST3" direction="pwr"/>
<pin name="GND/TEST4" direction="pwr"/>
<pin name="PA4/!FWR"/>
<pin name="PA5/!FRD"/>
</symbol>
<symbol name="EZ-USB-2122T">
<pin name="XOUT" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="SCL" direction="oc"/>
<pin name="SDA" direction="oc"/>
<pin name="RESET" direction="in"/>
<pin name="PA6/RXD0OUT"/>
<pin name="PA7/RXD1OUT"/>
<pin name="PB0/T2"/>
<pin name="PB1/T2EX"/>
<pin name="PB2/RXD1"/>
<pin name="PB3/TXD1"/>
<pin name="PB4/INT4"/>
<pin name="PB5/!INT5"/>
<pin name="PA0/T0OUT"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="!DISCON" direction="out"/>
<pin name="USBD+" direction="hiz"/>
<pin name="USBD-" direction="hiz"/>
<pin name="BKPT" direction="out"/>
<pin name="PB6/INT6"/>
<pin name="PB7/T2OUT"/>
<pin name="PC0/RXD0"/>
<pin name="PC1/TXD0"/>
<pin name="PC2/!INT0"/>
<pin name="PC3/!INT1"/>
<pin name="PC4/T0"/>
<pin name="PC5/T1"/>
<pin name="PC6/!WR"/>
<pin name="PC7/!RD"/>
<pin name="CLK24" direction="out"/>
<pin name="!WAKEUP" direction="in"/>
<pin name="CPU12MHZ" direction="in"/>
<pin name="VCC3.3@1" direction="pwr"/>
<pin name="VCC3.3@2" direction="pwr"/>
<pin name="VCC3.3@3" direction="pwr"/>
<pin name="VCC3.3@4" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND/TEST" direction="pwr"/>
<pin name="GND/TEST1" direction="pwr"/>
<pin name="GND/TEST2" direction="pwr"/>
<pin name="GND/TEST3" direction="pwr"/>
<pin name="GND/TEST4" direction="pwr"/>
<pin name="PA4/!FWR"/>
<pin name="PA5/!FRD"/>
</symbol>
<symbol name="EZ-USB-2125S">
<pin name="XOUT" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="SCL" direction="oc"/>
<pin name="SDA" direction="oc"/>
<pin name="RESET" direction="in"/>
<pin name="PA4/!FRW"/>
<pin name="PA5/!FRD"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="!DISCON" direction="out"/>
<pin name="USBD+" direction="hiz"/>
<pin name="USBD-" direction="hiz"/>
<pin name="BKPT" direction="out"/>
<pin name="PC0/RXD0"/>
<pin name="PC1/TXD0"/>
<pin name="PC2/!INT0"/>
<pin name="PC3/!INT1"/>
<pin name="PC4/T0"/>
<pin name="PC5/T1"/>
<pin name="PC6/!WR"/>
<pin name="PC7/!RD"/>
<pin name="CLK24" direction="out"/>
<pin name="!WAKEUP" direction="in"/>
<pin name="VCC3.3@1" direction="pwr"/>
<pin name="VCC3.3@2" direction="pwr"/>
<pin name="VCC3.3@3" direction="pwr"/>
<pin name="VCC3.3@4" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND/TEST" direction="pwr"/>
<pin name="GND/TEST1" direction="pwr"/>
<pin name="GND/TEST2" direction="pwr"/>
<pin name="GND/TEST3" direction="pwr"/>
<pin name="GND/TEST4" direction="pwr"/>
</symbol>
<symbol name="EZ-USB-2121S">
<pin name="XOUT" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="SCL" direction="oc"/>
<pin name="SDA" direction="oc"/>
<pin name="RESET" direction="in"/>
<pin name="PA4/!FRW"/>
<pin name="PA5/!FRD"/>
<pin name="PB0/T2"/>
<pin name="PB1/T2EX"/>
<pin name="PB2/RXD1"/>
<pin name="PB3/TXD1"/>
<pin name="PB4/INT4"/>
<pin name="PB5/!INT5"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="!DISCON" direction="out"/>
<pin name="USBD+" direction="hiz"/>
<pin name="USBD-" direction="hiz"/>
<pin name="BKPT" direction="out"/>
<pin name="PB6/INT6"/>
<pin name="PB7/T2OUT"/>
<pin name="PC0/RXD0"/>
<pin name="PC1/TXD0"/>
<pin name="PC2/!INT0"/>
<pin name="PC3/!INT1"/>
<pin name="PC4/T0"/>
<pin name="PC5/T1"/>
<pin name="PC6/!WR"/>
<pin name="PC7/!RD"/>
<pin name="CLK24" direction="out"/>
<pin name="!WAKEUP" direction="in"/>
<pin name="VCC3.3@1" direction="pwr"/>
<pin name="VCC3.3@2" direction="pwr"/>
<pin name="VCC3.3@3" direction="pwr"/>
<pin name="VCC3.3@4" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND/TEST" direction="pwr"/>
<pin name="GND/TEST1" direction="pwr"/>
<pin name="GND/TEST2" direction="pwr"/>
<pin name="GND/TEST3" direction="pwr"/>
<pin name="GND/TEST4" direction="pwr"/>
</symbol>
<symbol name="CYWUSB6934">
<pin name="RFOUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="DIOVAL"/>
<pin name="DIO"/>
<pin name="IRQ" direction="hiz"/>
<pin name="!SS" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="hiz"/>
<pin name="SCK" direction="in"/>
<pin name="X13OUT" direction="out"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="!PD" direction="in"/>
<pin name="PACTL"/>
<pin name="X13IN" direction="in"/>
<pin name="X13" direction="in"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="VCC@7" direction="pwr"/>
<pin name="VCC@8" direction="pwr"/>
<pin name="VCC@9" direction="pwr"/>
<pin name="RFIN" direction="in"/>
<pin name="GND@EXP" direction="pwr"/>
</symbol>
<symbol name="CYWUSB6932">
<pin name="RFOUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="DIOVAL"/>
<pin name="DIO"/>
<pin name="IRQ" direction="hiz"/>
<pin name="!SS" direction="in"/>
<pin name="MOSI" direction="in"/>
<pin name="MISO" direction="hiz"/>
<pin name="SCK" direction="in"/>
<pin name="X13OUT" direction="out"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="!PD" direction="in"/>
<pin name="PACTL"/>
<pin name="X13IN" direction="in"/>
<pin name="X13" direction="in"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="VCC@7" direction="pwr"/>
<pin name="VCC@8" direction="pwr"/>
<pin name="VCC@9" direction="pwr"/>
<pin name="GND@EXP" direction="pwr"/>
</symbol>
<symbol name="CY7C68013A-128">
<pin name="CLKOUT" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="RDY0/SLRD" direction="in"/>
<pin name="RDY1/SLRW" direction="in"/>
<pin name="RDY2" direction="in"/>
<pin name="RDY3" direction="in"/>
<pin name="RDY4" direction="in"/>
<pin name="RDY5" direction="in"/>
<pin name="AVCC" direction="in"/>
<pin name="XTALOUT" direction="in"/>
<pin name="XTALIN" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="AVCC@1" direction="in"/>
<pin name="DPLUS"/>
<pin name="DMINUS"/>
<pin name="AGND@1" direction="in"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="VCC@1" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="INT4" direction="out"/>
<pin name="T0" direction="out"/>
<pin name="T1" direction="out"/>
<pin name="T2" direction="out"/>
<pin name="IFCLK"/>
<pin name="RESEVED" direction="in"/>
<pin name="BKPT" direction="out"/>
<pin name="EA" direction="in"/>
<pin name="SCL" direction="out"/>
<pin name="SDA"/>
<pin name="!OE" direction="out"/>
<pin name="!PSEN" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="!WR" direction="out"/>
<pin name="!CS" direction="out"/>
<pin name="VCC@2" direction="in"/>
<pin name="PB0/FD0"/>
<pin name="PB1/FD1"/>
<pin name="PB2/FD2"/>
<pin name="PB3/FD3"/>
<pin name="VCC@3" direction="in"/>
<pin name="GND@3" direction="in"/>
<pin name="TXD0" direction="in"/>
<pin name="TXD1" direction="in"/>
<pin name="RXD0" direction="out"/>
<pin name="RXD1" direction="out"/>
<pin name="PB4/FD4"/>
<pin name="PB5/FD5"/>
<pin name="PB6/FD6"/>
<pin name="PB7/FD7"/>
<pin name="GND@4" direction="in"/>
<pin name="VCC@4" direction="in"/>
<pin name="GND@5" direction="in"/>
<pin name="VCC@5" direction="in"/>
<pin name="CTL3" direction="in"/>
<pin name="CTL4" direction="in"/>
<pin name="CTL0/FLAGA" direction="out"/>
<pin name="CTL1/FLAGB" direction="out"/>
<pin name="CTL2/FLAGC" direction="out"/>
<pin name="PC0/GPIFADR0"/>
<pin name="PC1/GPIFADR1"/>
<pin name="PC2/GPIFADR2"/>
<pin name="PC3/GPIFADR3"/>
<pin name="PC4/GPIFADR4"/>
<pin name="PC5/GPIFADR5"/>
<pin name="PC6/GPIFADR6"/>
<pin name="PC7/GPIFADR7"/>
<pin name="PA0/!INT0"/>
<pin name="PA1/!INT1"/>
<pin name="PA2/SLOE"/>
<pin name="PA3/WU2"/>
<pin name="PA4/FIFOADR0"/>
<pin name="PA5/FIFOADR1"/>
<pin name="PA6/PKTEND"/>
<pin name="PA7/FLAGD/!SLCS"/>
<pin name="CTL5"/>
<pin name="!RESET"/>
<pin name="PD0/FD8"/>
<pin name="PD1/FD9"/>
<pin name="PD2/FD10"/>
<pin name="PD3/FD11"/>
<pin name="PD4/FD12"/>
<pin name="PD5/FD13"/>
<pin name="PD6/FD14"/>
<pin name="PD7/FD15"/>
<pin name="!INT5" direction="out"/>
<pin name="PE0/T0OUT"/>
<pin name="PE1/T1OUT"/>
<pin name="PE2/T2OUT"/>
<pin name="PE3/RXD0OUT"/>
<pin name="PE4/RXD1OUT"/>
<pin name="PE5/INT6"/>
<pin name="PE6/T2EX"/>
<pin name="PE7/GPIFADR8"/>
<pin name="WAKEUP" direction="in"/>
<pin name="VCC@6" direction="in"/>
<pin name="VCC@7" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="GND@6" direction="in"/>
<pin name="VCC@8" direction="in"/>
<pin name="GND@7" direction="in"/>
<pin name="GND@8" direction="in"/>
</symbol>
<symbol name="CY7C68013A-100">
<pin name="CLKOUT" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="RDY0/SLRD" direction="in"/>
<pin name="RDY1/SLRW" direction="in"/>
<pin name="RDY2" direction="in"/>
<pin name="RDY3" direction="in"/>
<pin name="RDY4" direction="in"/>
<pin name="RDY5" direction="in"/>
<pin name="AVCC" direction="in"/>
<pin name="XTALOUT" direction="in"/>
<pin name="XTALIN" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="AVCC@1" direction="in"/>
<pin name="DPLUS"/>
<pin name="DMINUS"/>
<pin name="AGND@1" direction="in"/>
<pin name="VCC@1" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="INT4" direction="out"/>
<pin name="T0" direction="out"/>
<pin name="T1" direction="out"/>
<pin name="T2" direction="out"/>
<pin name="IFCLK"/>
<pin name="RESEVED" direction="in"/>
<pin name="BKPT" direction="out"/>
<pin name="SCL" direction="out"/>
<pin name="SDA"/>
<pin name="!RD" direction="out"/>
<pin name="!WR" direction="out"/>
<pin name="VCC@2" direction="in"/>
<pin name="PB0/FD0"/>
<pin name="PB1/FD1"/>
<pin name="PB2/FD2"/>
<pin name="PB3/FD3"/>
<pin name="VCC@3" direction="in"/>
<pin name="GND@3" direction="in"/>
<pin name="TXD0" direction="in"/>
<pin name="TXD1" direction="in"/>
<pin name="RXD0" direction="out"/>
<pin name="RXD1" direction="out"/>
<pin name="PB4/FD4"/>
<pin name="PB5/FD5"/>
<pin name="PB6/FD6"/>
<pin name="PB7/FD7"/>
<pin name="GND@4" direction="in"/>
<pin name="VCC@4" direction="in"/>
<pin name="GND@5" direction="in"/>
<pin name="VCC@5" direction="in"/>
<pin name="CTL3" direction="in"/>
<pin name="CTL4" direction="in"/>
<pin name="CTL0/FLAGA" direction="out"/>
<pin name="CTL1/FLAGB" direction="out"/>
<pin name="CTL2/FLAGC" direction="out"/>
<pin name="PC0/GPIFADR0"/>
<pin name="PC1/GPIFADR1"/>
<pin name="PC2/GPIFADR2"/>
<pin name="PC3/GPIFADR3"/>
<pin name="PC4/GPIFADR4"/>
<pin name="PC5/GPIFADR5"/>
<pin name="PC6/GPIFADR6"/>
<pin name="PC7/GPIFADR7"/>
<pin name="PA0/!INT0"/>
<pin name="PA1/!INT1"/>
<pin name="PA2/SLOE"/>
<pin name="PA3/WU2"/>
<pin name="PA4/FIFOADR0"/>
<pin name="PA5/FIFOADR1"/>
<pin name="PA6/PKTEND"/>
<pin name="PA7/FLAGD/!SLCS"/>
<pin name="CTL5"/>
<pin name="!RESET"/>
<pin name="PD0/FD8"/>
<pin name="PD1/FD9"/>
<pin name="PD2/FD10"/>
<pin name="PD3/FD11"/>
<pin name="PD4/FD12"/>
<pin name="PD5/FD13"/>
<pin name="PD6/FD14"/>
<pin name="PD7/FD15"/>
<pin name="!INT5" direction="out"/>
<pin name="PE0/T0OUT"/>
<pin name="PE1/T1OUT"/>
<pin name="PE2/T2OUT"/>
<pin name="PE3/RXD0OUT"/>
<pin name="PE4/RXD1OUT"/>
<pin name="PE5/INT6"/>
<pin name="PE6/T2EX"/>
<pin name="PE7/GPIFADR8"/>
<pin name="WAKEUP" direction="in"/>
<pin name="VCC@6" direction="in"/>
<pin name="VCC@7" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="GND@6" direction="in"/>
<pin name="VCC@8" direction="in"/>
<pin name="GND@7" direction="in"/>
<pin name="GND@8" direction="in"/>
</symbol>
<symbol name="CY7C68013A-56">
<pin name="CLKOUT/T1OUT" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="RDY0/SLRD" direction="in"/>
<pin name="RDY1/SLRW" direction="in"/>
<pin name="AVCC" direction="in"/>
<pin name="XTALOUT" direction="in"/>
<pin name="XTALIN" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="AVCC@1" direction="in"/>
<pin name="DPLUS"/>
<pin name="DMINUS"/>
<pin name="AGND@1" direction="in"/>
<pin name="VCC@1" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="IFCLK/T0OUT"/>
<pin name="RESEVED" direction="in"/>
<pin name="SCL" direction="out"/>
<pin name="SDA"/>
<pin name="VCC@2" direction="in"/>
<pin name="PB0/FD0"/>
<pin name="PB1/FD1"/>
<pin name="PB2/FD2"/>
<pin name="PB3/FD3"/>
<pin name="VCC@3" direction="in"/>
<pin name="GND@3" direction="in"/>
<pin name="PB4/FD4"/>
<pin name="PB5/FD5"/>
<pin name="PB6/FD6"/>
<pin name="PB7/FD7"/>
<pin name="GND@4" direction="in"/>
<pin name="VCC@4" direction="in"/>
<pin name="GND@5" direction="in"/>
<pin name="VCC@5" direction="in"/>
<pin name="CTL0/FLAGA" direction="out"/>
<pin name="CTL1/FLAGB" direction="out"/>
<pin name="CTL2/FLAGC" direction="out"/>
<pin name="PA0/!INT0"/>
<pin name="PA1/!INT1"/>
<pin name="PA2/SLOE"/>
<pin name="PA3/WU2"/>
<pin name="PA4/FIFOADR0"/>
<pin name="PA5/FIFOADR1"/>
<pin name="PA6/PKTEND"/>
<pin name="PA7/FLAGD/!SLCS"/>
<pin name="PD0/FD8"/>
<pin name="PD1/FD9"/>
<pin name="PD2/FD10"/>
<pin name="PD3/FD11"/>
<pin name="PD4/FD12"/>
<pin name="PD5/FD13"/>
<pin name="PD6/FD14"/>
<pin name="PD7/FD15"/>
<pin name="WAKEUP" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="!RESET" direction="in"/>
</symbol>
<symbol name="CY7C68013A-56QFN">
<pin name="CLKOUT/T1OUT" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="RDY0/SLRD" direction="in"/>
<pin name="RDY1/SLRW" direction="in"/>
<pin name="AVCC" direction="in"/>
<pin name="XTALOUT" direction="in"/>
<pin name="XTALIN" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="AVCC@1" direction="in"/>
<pin name="DPLUS"/>
<pin name="DMINUS"/>
<pin name="AGND@1" direction="in"/>
<pin name="VCC@1" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="IFCLK/T0OUT"/>
<pin name="RESEVED" direction="in"/>
<pin name="SCL" direction="out"/>
<pin name="SDA"/>
<pin name="VCC@2" direction="in"/>
<pin name="PB0/FD0"/>
<pin name="PB1/FD1"/>
<pin name="PB2/FD2"/>
<pin name="PB3/FD3"/>
<pin name="VCC@3" direction="in"/>
<pin name="GND@3" direction="in"/>
<pin name="PB4/FD4"/>
<pin name="PB5/FD5"/>
<pin name="PB6/FD6"/>
<pin name="PB7/FD7"/>
<pin name="GND@4" direction="in"/>
<pin name="VCC@4" direction="in"/>
<pin name="GND@5" direction="in"/>
<pin name="VCC@5" direction="in"/>
<pin name="CTL0/FLAGA" direction="out"/>
<pin name="CTL1/FLAGB" direction="out"/>
<pin name="CTL2/FLAGC" direction="out"/>
<pin name="PA0/!INT0"/>
<pin name="PA1/!INT1"/>
<pin name="PA2/SLOE"/>
<pin name="PA3/WU2"/>
<pin name="PA4/FIFOADR0"/>
<pin name="PA5/FIFOADR1"/>
<pin name="PA6/PKTEND"/>
<pin name="PA7/FLAGD/!SLCS"/>
<pin name="PD0/FD8"/>
<pin name="PD1/FD9"/>
<pin name="PD2/FD10"/>
<pin name="PD3/FD11"/>
<pin name="PD4/FD12"/>
<pin name="PD5/FD13"/>
<pin name="PD6/FD14"/>
<pin name="PD7/FD15"/>
<pin name="WAKEUP" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="EPAD" direction="pas"/>
</symbol>
<symbol name="CY7C63001">
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="CEXT" direction="pas"/>
<pin name="XTALOUT" direction="out"/>
<pin name="XTALIN" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VPP" direction="in"/>
</symbol>
<symbol name="CY7C63101C-QXC">
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="CEXT" direction="pas"/>
<pin name="XTALOUT" direction="out"/>
<pin name="XTALIN" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="VPP" direction="in"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
</symbol>
<symbol name="CY8C22345">
<pin name="AI/MR/P0[7]"/>
<pin name="AI/ML/P0[5]"/>
<pin name="AI/ML/P0[3]"/>
<pin name="AI/ML/P0[1]"/>
<pin name="P0[6]/MR/AI"/>
<pin name="P0[4]/MR/AI"/>
<pin name="P0[2]/MR/AI"/>
<pin name="P0[0]/MR/AI"/>
<pin name="AI/ML/P2[7]"/>
<pin name="ADC_VREF/ML/P2[5]"/>
<pin name="ML/P2[3]"/>
<pin name="ML/P2[1]"/>
<pin name="P2[6]/MR/AI"/>
<pin name="P2[4]/MR"/>
<pin name="P2[2]/MR"/>
<pin name="P2[0]/MR"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="XRES" direction="in"/>
<pin name="I2C_SCL/ML/P1[7]"/>
<pin name="I2C_SDA/ML/P1[5]"/>
<pin name="ML/P1[3]"/>
<pin name="I2C_SCL/ML/P1[1]"/>
<pin name="P1[0]/MR/I2C_SDA"/>
<pin name="P1[2]/MR"/>
<pin name="P1[4]/MR/EXTCLK"/>
<pin name="P1[6]/MR"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="CY8C22545">
<pin name="ADC_VREF/ML/P2[5]"/>
<pin name="ML/P2[3]"/>
<pin name="ML/P2[1]"/>
<pin name="ML/P4[5]"/>
<pin name="ML/P4[3]"/>
<pin name="ML/P4[1]"/>
<pin name="ML/P3[7]"/>
<pin name="ML/P3[5]"/>
<pin name="ML/P3[3]"/>
<pin name="ML/P3[1]"/>
<pin name="I2C_SCL/ML/P1[7]"/>
<pin name="I2C_SDA/ML/P1[5]"/>
<pin name="ML/P1[3]"/>
<pin name="I2C_SCL/XTALIN/ML/P1[1]"/>
<pin name="I2C_SCA/XTALOUT/MR/P1[0]"/>
<pin name="MR/P1[2]"/>
<pin name="EXTCLK/MR/P1[4]"/>
<pin name="MR/P1[6]"/>
<pin name="MR/P3[0]"/>
<pin name="MR/P3[2]"/>
<pin name="MR/P3[4]"/>
<pin name="MR/P3[6]"/>
<pin name="MR/P4[0]"/>
<pin name="MR/P4[2]"/>
<pin name="MR/P4[4]"/>
<pin name="MR/P2[0]"/>
<pin name="MR/P2[2]"/>
<pin name="MR/P2[4]"/>
<pin name="AI/MR/P2[6]"/>
<pin name="AI/MR/P0[0]"/>
<pin name="AI/MR/P0[2]"/>
<pin name="AI/MR/P0[4]"/>
<pin name="AI/MR/P0[6]"/>
<pin name="AI/MR/P0[7]"/>
<pin name="AI/ML/P0[5]"/>
<pin name="AI/ML/P0[3]"/>
<pin name="AI/ML/P0[1]"/>
<pin name="AI/ML/P2[7]"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="XRES" direction="in"/>
</symbol>
<symbol name="CY8C21234">
<pin name="A/I/M/P0[7]"/>
<pin name="A/I/M/P0[5]"/>
<pin name="A/I/M/P0[3]"/>
<pin name="A/I/M/P0[1]"/>
<pin name="P0[6]/M/I/A"/>
<pin name="P0[4]/M/I/A"/>
<pin name="P0[2]/M/I/A"/>
<pin name="P0[0]/M/I/A"/>
<pin name="P1[4]/EXTCLK/M"/>
<pin name="P1[2]/M"/>
<pin name="P1[0]/I2C_SDA/M"/>
<pin name="M/I2C_SCL/P1[1]"/>
<pin name="SMP" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="CY8C21334">
<pin name="A/I/M/P0[7]"/>
<pin name="A/I/M/P0[5]"/>
<pin name="A/I/M/P0[3]"/>
<pin name="A/I/M/P0[1]"/>
<pin name="P0[6]/M/I/A"/>
<pin name="P0[4]/M/I/A"/>
<pin name="P0[2]/M/I/A"/>
<pin name="P0[0]/M/I/A"/>
<pin name="P1[6]/M"/>
<pin name="P1[4]/EXT_CLK/M"/>
<pin name="M/I2C_SCL/P1[7]"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="M/I2C_SDA/P1[5]"/>
<pin name="MP1[3]"/>
<pin name="M/I2C_SCL/P1[1]"/>
<pin name="P1[2]/M"/>
<pin name="P1[0]/I2C_SDA/M"/>
<pin name="XRES" direction="in"/>
</symbol>
<symbol name="CY8C21534">
<pin name="A/I/M/P0[7]"/>
<pin name="A/I/M/P0[5]"/>
<pin name="A/I/M/P0[3]"/>
<pin name="A/I/M/P0[1]"/>
<pin name="M/P2[7]"/>
<pin name="M/P2[5]"/>
<pin name="M/P2[3]"/>
<pin name="M/P2[1]"/>
<pin name="M/I2C_SCL/P1[7]"/>
<pin name="M/I2C_SDA/P1[5]"/>
<pin name="M/P1[3]"/>
<pin name="M/I2C_SCL/P1[1]"/>
<pin name="P1[0]/I2C_SDA/M"/>
<pin name="P1[2]/M"/>
<pin name="P1[4]/EXTCLK/M"/>
<pin name="P1[6]/M"/>
<pin name="P2[0]/M"/>
<pin name="P2[2]/M"/>
<pin name="P2[4]/M"/>
<pin name="P2[6]/M"/>
<pin name="P0[0]/A/I/M"/>
<pin name="P0[2]/A/I/M"/>
<pin name="P0[4]/A/I/M"/>
<pin name="P0[6]/A/I/M"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="XRES" direction="in"/>
</symbol>
<symbol name="CY8C21434">
<pin name="A/I/M/P0[1]"/>
<pin name="M/P2[7]"/>
<pin name="M/P2[5]"/>
<pin name="M/P2[3]"/>
<pin name="M/P2[1]"/>
<pin name="M/P3[3]"/>
<pin name="M/P3[1]"/>
<pin name="M/12C_SCL/P1[7]"/>
<pin name="M/I2C_SDA/P1[5]"/>
<pin name="M/P1[3]"/>
<pin name="M/I2C_SCL/P1[1]"/>
<pin name="M/I2C_SDA/P1[0]"/>
<pin name="M/P1[2]"/>
<pin name="M/EXTCLK/P1[4]"/>
<pin name="M/P1[6]"/>
<pin name="P3[0]/M"/>
<pin name="P3[2]/M"/>
<pin name="P2[0]/M"/>
<pin name="P2[2]/M"/>
<pin name="P2[4]/M"/>
<pin name="P2[6]/M"/>
<pin name="P0[0]/A/I/M"/>
<pin name="P0[2]/A/I/M"/>
<pin name="P0[4]/A/I/M"/>
<pin name="P0[6]/A/I/M"/>
<pin name="P0[7]/A/I/M"/>
<pin name="P0[5]/A/I/M"/>
<pin name="P0[3]/A/I/M"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="XRES" direction="in"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="CY8C21634">
<pin name="A/I/M/P0[1]"/>
<pin name="M/P2[7]"/>
<pin name="M/P2[5]"/>
<pin name="M/P2[3]"/>
<pin name="M/P2[1]"/>
<pin name="SMP" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="M/12C_SCL/P1[7]"/>
<pin name="M/I2C_SDA/P1[5]"/>
<pin name="M/P1[3]"/>
<pin name="M/I2C_SCL/P1[1]"/>
<pin name="M/I2C_SDA/P1[0]"/>
<pin name="M/P1[2]"/>
<pin name="M/EXTCLK/P1[4]"/>
<pin name="M/P1[6]"/>
<pin name="P3[0]/M"/>
<pin name="P3[2]/M"/>
<pin name="P2[0]/M"/>
<pin name="P2[2]/M"/>
<pin name="P2[4]/M"/>
<pin name="P2[6]/M"/>
<pin name="P0[0]/A/I/M"/>
<pin name="P0[2]/A/I/M"/>
<pin name="P0[4]/A/I/M"/>
<pin name="P0[6]/A/I/M"/>
<pin name="P0[7]/A/I/M"/>
<pin name="P0[5]/A/I/M"/>
<pin name="P0[3]/A/I/M"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="XRES" direction="in"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="CY8C58LPXXX_TQFP100_4JTAG">
<pin name="P2_5"/>
<pin name="P2_6"/>
<pin name="P2_7"/>
<pin name="P12_4"/>
<pin name="P12_5"/>
<pin name="P6_4"/>
<pin name="P6_5"/>
<pin name="P6_6"/>
<pin name="P6_7"/>
<pin name="VSSB" direction="pwr"/>
<pin name="IND" direction="pas"/>
<pin name="VB" direction="pas"/>
<pin name="VBAT" direction="pas"/>
<pin name="VSSD@0" direction="pwr"/>
<pin name="XRES_N" direction="in"/>
<pin name="P5_0"/>
<pin name="P5_1"/>
<pin name="P5_2"/>
<pin name="P5_3"/>
<pin name="P1_0" direction="in"/>
<pin name="P1_1" direction="in"/>
<pin name="P1_2"/>
<pin name="P1_3" direction="out"/>
<pin name="P1_4" direction="in"/>
<pin name="P1_5"/>
<pin name="VIO1" direction="pas"/>
<pin name="P1_6"/>
<pin name="P1_7"/>
<pin name="P12_6"/>
<pin name="P12_7"/>
<pin name="P5_4"/>
<pin name="P5_5"/>
<pin name="P5_6"/>
<pin name="P5_7"/>
<pin name="P15_6" direction="hiz"/>
<pin name="P15_7" direction="hiz"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VSSD@0@1" direction="pwr"/>
<pin name="VCCD@0" direction="pwr"/>
<pin name="P15_0"/>
<pin name="P15_1"/>
<pin name="P3_0"/>
<pin name="P3_1"/>
<pin name="P3_2"/>
<pin name="P3_3"/>
<pin name="P3_4"/>
<pin name="P3_5"/>
<pin name="VIO3" direction="pas"/>
<pin name="P3_6"/>
<pin name="P3_7"/>
<pin name="P12_0"/>
<pin name="P12_1"/>
<pin name="P15_2"/>
<pin name="P15_3"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSD@1" direction="pwr"/>
<pin name="P12_2"/>
<pin name="P12_3"/>
<pin name="P4_0"/>
<pin name="P4_1"/>
<pin name="P0_0"/>
<pin name="P0_1"/>
<pin name="P0_2"/>
<pin name="P0_3"/>
<pin name="VIO0" direction="pas"/>
<pin name="P0_4"/>
<pin name="P0_5"/>
<pin name="P0_6"/>
<pin name="P0_7"/>
<pin name="P4_2"/>
<pin name="P4_3"/>
<pin name="P4_4"/>
<pin name="P4_5"/>
<pin name="P4_6"/>
<pin name="P4_7"/>
<pin name="VCCD@1" direction="pwr"/>
<pin name="VSSD@1@1" direction="pwr"/>
<pin name="VDDD@1" direction="pwr"/>
<pin name="P6_0"/>
<pin name="P6_1"/>
<pin name="P6_2"/>
<pin name="P6_3"/>
<pin name="P15_4"/>
<pin name="P15_5"/>
<pin name="P2_0"/>
<pin name="P2_1"/>
<pin name="P2_2"/>
<pin name="P2_3"/>
<pin name="P2_4"/>
<pin name="VIO2" direction="pas"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
</symbol>
<symbol name="CY8C58LPXXX_TQFP100_5JTAG">
<pin name="P2_5"/>
<pin name="P2_6"/>
<pin name="P2_7"/>
<pin name="P12_4"/>
<pin name="P12_5"/>
<pin name="P6_4"/>
<pin name="P6_5"/>
<pin name="P6_6"/>
<pin name="P6_7"/>
<pin name="VSSB" direction="pwr"/>
<pin name="IND" direction="pas"/>
<pin name="VB" direction="pas"/>
<pin name="VBAT" direction="pas"/>
<pin name="VSSD@0" direction="pwr"/>
<pin name="XRES_N" direction="in"/>
<pin name="P5_0"/>
<pin name="P5_1"/>
<pin name="P5_2"/>
<pin name="P5_3"/>
<pin name="P1_0" direction="in"/>
<pin name="P1_1" direction="in"/>
<pin name="P1_2"/>
<pin name="P1_3" direction="out"/>
<pin name="P1_4" direction="in"/>
<pin name="P1_5" direction="in"/>
<pin name="VIO1" direction="pas"/>
<pin name="P1_6"/>
<pin name="P1_7"/>
<pin name="P12_6"/>
<pin name="P12_7"/>
<pin name="P5_4"/>
<pin name="P5_5"/>
<pin name="P5_6"/>
<pin name="P5_7"/>
<pin name="P15_6" direction="hiz"/>
<pin name="P15_7" direction="hiz"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VSSD@0@1" direction="pwr"/>
<pin name="VCCD@0" direction="pwr"/>
<pin name="P15_0"/>
<pin name="P15_1"/>
<pin name="P3_0"/>
<pin name="P3_1"/>
<pin name="P3_2"/>
<pin name="P3_3"/>
<pin name="P3_4"/>
<pin name="P3_5"/>
<pin name="VIO3" direction="pas"/>
<pin name="P3_6"/>
<pin name="P3_7"/>
<pin name="P12_0"/>
<pin name="P12_1"/>
<pin name="P15_2"/>
<pin name="P15_3"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSD@1" direction="pwr"/>
<pin name="P12_2"/>
<pin name="P12_3"/>
<pin name="P4_0"/>
<pin name="P4_1"/>
<pin name="P0_0"/>
<pin name="P0_1"/>
<pin name="P0_2"/>
<pin name="P0_3"/>
<pin name="VIO0" direction="pas"/>
<pin name="P0_4"/>
<pin name="P0_5"/>
<pin name="P0_6"/>
<pin name="P0_7"/>
<pin name="P4_2"/>
<pin name="P4_3"/>
<pin name="P4_4"/>
<pin name="P4_5"/>
<pin name="P4_6"/>
<pin name="P4_7"/>
<pin name="VCCD@1" direction="pwr"/>
<pin name="VSSD@1@1" direction="pwr"/>
<pin name="VDDD@1" direction="pwr"/>
<pin name="P6_0"/>
<pin name="P6_1"/>
<pin name="P6_2"/>
<pin name="P6_3"/>
<pin name="P15_4"/>
<pin name="P15_5"/>
<pin name="P2_0"/>
<pin name="P2_1"/>
<pin name="P2_2"/>
<pin name="P2_3"/>
<pin name="P2_4"/>
<pin name="VIO2" direction="pas"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
</symbol>
<symbol name="CY8C58LPXXX_TQFP100_USB_4JTAG">
<pin name="P2_5"/>
<pin name="P2_6"/>
<pin name="P2_7"/>
<pin name="P12_4"/>
<pin name="P12_5"/>
<pin name="P6_4"/>
<pin name="P6_5"/>
<pin name="P6_6"/>
<pin name="P6_7"/>
<pin name="VSSB" direction="pwr"/>
<pin name="IND" direction="pas"/>
<pin name="VB" direction="pas"/>
<pin name="VBAT" direction="pas"/>
<pin name="VSSD@0" direction="pwr"/>
<pin name="XRES_N" direction="in"/>
<pin name="P5_0"/>
<pin name="P5_1"/>
<pin name="P5_2"/>
<pin name="P5_3"/>
<pin name="P1_0" direction="in"/>
<pin name="P1_1" direction="in"/>
<pin name="P1_2"/>
<pin name="P1_3" direction="out"/>
<pin name="P1_4" direction="in"/>
<pin name="P1_5"/>
<pin name="VIO1" direction="pas"/>
<pin name="P1_6"/>
<pin name="P1_7"/>
<pin name="P12_6"/>
<pin name="P12_7"/>
<pin name="P5_4"/>
<pin name="P5_5"/>
<pin name="P5_6"/>
<pin name="P5_7"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VSSD@0@1" direction="pwr"/>
<pin name="VCCD@0" direction="pwr"/>
<pin name="P15_0"/>
<pin name="P15_1"/>
<pin name="P3_0"/>
<pin name="P3_1"/>
<pin name="P3_2"/>
<pin name="P3_3"/>
<pin name="P3_4"/>
<pin name="P3_5"/>
<pin name="VIO3" direction="pas"/>
<pin name="P3_6"/>
<pin name="P3_7"/>
<pin name="P12_0"/>
<pin name="P12_1"/>
<pin name="P15_2"/>
<pin name="P15_3"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSD@1" direction="pwr"/>
<pin name="P12_2"/>
<pin name="P12_3"/>
<pin name="P4_0"/>
<pin name="P4_1"/>
<pin name="P0_0"/>
<pin name="P0_1"/>
<pin name="P0_2"/>
<pin name="P0_3"/>
<pin name="VIO0" direction="pas"/>
<pin name="P0_4"/>
<pin name="P0_5"/>
<pin name="P0_6"/>
<pin name="P0_7"/>
<pin name="P4_2"/>
<pin name="P4_3"/>
<pin name="P4_4"/>
<pin name="P4_5"/>
<pin name="P4_6"/>
<pin name="P4_7"/>
<pin name="VCCD@1" direction="pwr"/>
<pin name="VSSD@1@1" direction="pwr"/>
<pin name="VDDD@1" direction="pwr"/>
<pin name="P6_0"/>
<pin name="P6_1"/>
<pin name="P6_2"/>
<pin name="P6_3"/>
<pin name="P15_4"/>
<pin name="P15_5"/>
<pin name="P2_0"/>
<pin name="P2_1"/>
<pin name="P2_2"/>
<pin name="P2_3"/>
<pin name="P2_4"/>
<pin name="VIO2" direction="pas"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="USB_D+" direction="hiz"/>
<pin name="USB_D-" direction="hiz"/>
</symbol>
<symbol name="CY8C58LPXXX_TQFP100_USB_5JTAG">
<pin name="P2_5"/>
<pin name="P2_6"/>
<pin name="P2_7"/>
<pin name="P12_4"/>
<pin name="P12_5"/>
<pin name="P6_4"/>
<pin name="P6_5"/>
<pin name="P6_6"/>
<pin name="P6_7"/>
<pin name="VSSB" direction="pwr"/>
<pin name="IND" direction="pas"/>
<pin name="VB" direction="pas"/>
<pin name="VBAT" direction="pas"/>
<pin name="VSSD@0" direction="pwr"/>
<pin name="XRES_N" direction="in"/>
<pin name="P5_0"/>
<pin name="P5_1"/>
<pin name="P5_2"/>
<pin name="P5_3"/>
<pin name="P1_0" direction="in"/>
<pin name="P1_1" direction="in"/>
<pin name="P1_2"/>
<pin name="P1_3" direction="out"/>
<pin name="P1_4" direction="in"/>
<pin name="P1_5" direction="in"/>
<pin name="VIO1" direction="pas"/>
<pin name="P1_6"/>
<pin name="P1_7"/>
<pin name="P12_6"/>
<pin name="P12_7"/>
<pin name="P5_4"/>
<pin name="P5_5"/>
<pin name="P5_6"/>
<pin name="P5_7"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VSSD@0@1" direction="pwr"/>
<pin name="VCCD@0" direction="pwr"/>
<pin name="P15_0"/>
<pin name="P15_1"/>
<pin name="P3_0"/>
<pin name="P3_1"/>
<pin name="P3_2"/>
<pin name="P3_3"/>
<pin name="P3_4"/>
<pin name="P3_5"/>
<pin name="VIO3" direction="pas"/>
<pin name="P3_6"/>
<pin name="P3_7"/>
<pin name="P12_0"/>
<pin name="P12_1"/>
<pin name="P15_2"/>
<pin name="P15_3"/>
<pin name="VCCA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSD@1" direction="pwr"/>
<pin name="P12_2"/>
<pin name="P12_3"/>
<pin name="P4_0"/>
<pin name="P4_1"/>
<pin name="P0_0"/>
<pin name="P0_1"/>
<pin name="P0_2"/>
<pin name="P0_3"/>
<pin name="VIO0" direction="pas"/>
<pin name="P0_4"/>
<pin name="P0_5"/>
<pin name="P0_6"/>
<pin name="P0_7"/>
<pin name="P4_2"/>
<pin name="P4_3"/>
<pin name="P4_4"/>
<pin name="P4_5"/>
<pin name="P4_6"/>
<pin name="P4_7"/>
<pin name="VCCD@1" direction="pwr"/>
<pin name="VSSD@1@1" direction="pwr"/>
<pin name="VDDD@1" direction="pwr"/>
<pin name="P6_0"/>
<pin name="P6_1"/>
<pin name="P6_2"/>
<pin name="P6_3"/>
<pin name="P15_4"/>
<pin name="P15_5"/>
<pin name="P2_0"/>
<pin name="P2_1"/>
<pin name="P2_2"/>
<pin name="P2_3"/>
<pin name="P2_4"/>
<pin name="VIO2" direction="pas"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="USB_D+" direction="hiz"/>
<pin name="USB_D-" direction="hiz"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="EZ-USB-2131Q" prefix="IC">
<description>Microcontroller with USB port</description>
<gates>
<gate name="G$1" symbol="EZ-USB-2131Q"/>
</gates>
<devices>
<device name="" package="PQFP80">
<connects>
<connect gate="G$1" pin="!DISCON" pad="1"/>
<connect gate="G$1" pin="!WAKEUP" pad="66"/>
<connect gate="G$1" pin="A0" pad="7"/>
<connect gate="G$1" pin="A1" pad="8"/>
<connect gate="G$1" pin="A10" pad="28"/>
<connect gate="G$1" pin="A11" pad="29"/>
<connect gate="G$1" pin="A12" pad="34"/>
<connect gate="G$1" pin="A13" pad="35"/>
<connect gate="G$1" pin="A14" pad="36"/>
<connect gate="G$1" pin="A15" pad="37"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="10"/>
<connect gate="G$1" pin="A4" pad="11"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="16"/>
<connect gate="G$1" pin="A8" pad="26"/>
<connect gate="G$1" pin="A9" pad="27"/>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="AVCC" pad="21"/>
<connect gate="G$1" pin="BKPT" pad="61"/>
<connect gate="G$1" pin="CLK24" pad="4"/>
<connect gate="G$1" pin="D0" pad="48"/>
<connect gate="G$1" pin="D1" pad="49"/>
<connect gate="G$1" pin="D2" pad="50"/>
<connect gate="G$1" pin="D3" pad="51"/>
<connect gate="G$1" pin="D4" pad="57"/>
<connect gate="G$1" pin="D5" pad="58"/>
<connect gate="G$1" pin="D6" pad="59"/>
<connect gate="G$1" pin="D7" pad="60"/>
<connect gate="G$1" pin="EA" pad="24"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND/TEST" pad="72"/>
<connect gate="G$1" pin="GND/TEST1" pad="5"/>
<connect gate="G$1" pin="GND/TEST2" pad="6"/>
<connect gate="G$1" pin="GND/TEST3" pad="13"/>
<connect gate="G$1" pin="GND/TEST4" pad="14"/>
<connect gate="G$1" pin="GND@1" pad="17"/>
<connect gate="G$1" pin="GND@2" pad="23"/>
<connect gate="G$1" pin="GND@3" pad="43"/>
<connect gate="G$1" pin="GND@4" pad="56"/>
<connect gate="G$1" pin="GND@5" pad="63"/>
<connect gate="G$1" pin="GND@6" pad="78"/>
<connect gate="G$1" pin="PA0/T0OUT" pad="68"/>
<connect gate="G$1" pin="PA1/T1OUT" pad="69"/>
<connect gate="G$1" pin="PA2/!OE" pad="70"/>
<connect gate="G$1" pin="PA3/!CS" pad="71"/>
<connect gate="G$1" pin="PA4/!FRW" pad="73"/>
<connect gate="G$1" pin="PA5/!FRD" pad="74"/>
<connect gate="G$1" pin="PA6/RXD0OUT" pad="75"/>
<connect gate="G$1" pin="PA7/RXD1OUT" pad="76"/>
<connect gate="G$1" pin="PB0/T2" pad="44"/>
<connect gate="G$1" pin="PB1/T2EX" pad="45"/>
<connect gate="G$1" pin="PB2/RXD1" pad="46"/>
<connect gate="G$1" pin="PB3/TXD1" pad="47"/>
<connect gate="G$1" pin="PB4/INT4" pad="52"/>
<connect gate="G$1" pin="PB5/!INT5" pad="53"/>
<connect gate="G$1" pin="PB6/INT6" pad="54"/>
<connect gate="G$1" pin="PB7/T2OUT" pad="55"/>
<connect gate="G$1" pin="PC0/RXD0" pad="30"/>
<connect gate="G$1" pin="PC1/TXD0" pad="31"/>
<connect gate="G$1" pin="PC2/!INT0" pad="32"/>
<connect gate="G$1" pin="PC3/!INT1" pad="33"/>
<connect gate="G$1" pin="PC4/T0" pad="38"/>
<connect gate="G$1" pin="PC5/T1" pad="39"/>
<connect gate="G$1" pin="PC6/!WR" pad="40"/>
<connect gate="G$1" pin="PC7/!RD" pad="41"/>
<connect gate="G$1" pin="PSEN" pad="80"/>
<connect gate="G$1" pin="RESET" pad="25"/>
<connect gate="G$1" pin="SCL" pad="65"/>
<connect gate="G$1" pin="SDA" pad="64"/>
<connect gate="G$1" pin="USBD+" pad="79"/>
<connect gate="G$1" pin="USBD-" pad="77"/>
<connect gate="G$1" pin="VCC3.3@1" pad="2"/>
<connect gate="G$1" pin="VCC3.3@2" pad="22"/>
<connect gate="G$1" pin="VCC3.3@3" pad="42"/>
<connect gate="G$1" pin="VCC3.3@4" pad="62"/>
<connect gate="G$1" pin="XIN" pad="19"/>
<connect gate="G$1" pin="XOUT" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EZ-USB-2*S" prefix="IC">
<description>Microcontroller with USB port</description>
<gates>
<gate name="G$1" symbol="EZ-USB-2121S"/>
</gates>
<devices>
<device name="" package="PQFP44">
<connects>
<connect gate="G$1" pin="!DISCON" pad="43"/>
<connect gate="G$1" pin="!WAKEUP" pad="37"/>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="AVCC" pad="10"/>
<connect gate="G$1" pin="BKPT" pad="32"/>
<connect gate="G$1" pin="CLK24" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND/TEST" pad="38"/>
<connect gate="G$1" pin="GND/TEST1" pad="3"/>
<connect gate="G$1" pin="GND/TEST2" pad="4"/>
<connect gate="G$1" pin="GND/TEST3" pad="5"/>
<connect gate="G$1" pin="GND/TEST4" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="23"/>
<connect gate="G$1" pin="GND@3" pad="34"/>
<connect gate="G$1" pin="PA4/!FRW" pad="39"/>
<connect gate="G$1" pin="PA5/!FRD" pad="40"/>
<connect gate="G$1" pin="PB0/T2" pad="24"/>
<connect gate="G$1" pin="PB1/T2EX" pad="25"/>
<connect gate="G$1" pin="PB2/RXD1" pad="26"/>
<connect gate="G$1" pin="PB3/TXD1" pad="27"/>
<connect gate="G$1" pin="PB4/INT4" pad="28"/>
<connect gate="G$1" pin="PB5/!INT5" pad="29"/>
<connect gate="G$1" pin="PB6/INT6" pad="30"/>
<connect gate="G$1" pin="PB7/T2OUT" pad="31"/>
<connect gate="G$1" pin="PC0/RXD0" pad="14"/>
<connect gate="G$1" pin="PC1/TXD0" pad="15"/>
<connect gate="G$1" pin="PC2/!INT0" pad="16"/>
<connect gate="G$1" pin="PC3/!INT1" pad="17"/>
<connect gate="G$1" pin="PC4/T0" pad="18"/>
<connect gate="G$1" pin="PC5/T1" pad="19"/>
<connect gate="G$1" pin="PC6/!WR" pad="20"/>
<connect gate="G$1" pin="PC7/!RD" pad="21"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="G$1" pin="SCL" pad="36"/>
<connect gate="G$1" pin="SDA" pad="35"/>
<connect gate="G$1" pin="USBD+" pad="42"/>
<connect gate="G$1" pin="USBD-" pad="41"/>
<connect gate="G$1" pin="VCC3.3@1" pad="11"/>
<connect gate="G$1" pin="VCC3.3@2" pad="22"/>
<connect gate="G$1" pin="VCC3.3@3" pad="33"/>
<connect gate="G$1" pin="VCC3.3@4" pad="44"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT" pad="9"/>
</connects>
<technologies>
<technology name="121">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="122">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="131">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EZ-USB-21*S" prefix="IC">
<description>Microcontroller with USB port</description>
<gates>
<gate name="G$1" symbol="EZ-USB-2125S"/>
</gates>
<devices>
<device name="" package="PQFP44">
<connects>
<connect gate="G$1" pin="!DISCON" pad="43"/>
<connect gate="G$1" pin="!WAKEUP" pad="37"/>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="AVCC" pad="10"/>
<connect gate="G$1" pin="BKPT" pad="32"/>
<connect gate="G$1" pin="CLK24" pad="2"/>
<connect gate="G$1" pin="D0" pad="24"/>
<connect gate="G$1" pin="D1" pad="25"/>
<connect gate="G$1" pin="D2" pad="26"/>
<connect gate="G$1" pin="D3" pad="27"/>
<connect gate="G$1" pin="D4" pad="28"/>
<connect gate="G$1" pin="D5" pad="29"/>
<connect gate="G$1" pin="D6" pad="30"/>
<connect gate="G$1" pin="D7" pad="31"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND/TEST" pad="38"/>
<connect gate="G$1" pin="GND/TEST1" pad="3"/>
<connect gate="G$1" pin="GND/TEST2" pad="4"/>
<connect gate="G$1" pin="GND/TEST3" pad="5"/>
<connect gate="G$1" pin="GND/TEST4" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="23"/>
<connect gate="G$1" pin="GND@3" pad="34"/>
<connect gate="G$1" pin="PA4/!FRW" pad="39"/>
<connect gate="G$1" pin="PA5/!FRD" pad="40"/>
<connect gate="G$1" pin="PC0/RXD0" pad="14"/>
<connect gate="G$1" pin="PC1/TXD0" pad="15"/>
<connect gate="G$1" pin="PC2/!INT0" pad="16"/>
<connect gate="G$1" pin="PC3/!INT1" pad="17"/>
<connect gate="G$1" pin="PC4/T0" pad="18"/>
<connect gate="G$1" pin="PC5/T1" pad="19"/>
<connect gate="G$1" pin="PC6/!WR" pad="20"/>
<connect gate="G$1" pin="PC7/!RD" pad="21"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="G$1" pin="SCL" pad="36"/>
<connect gate="G$1" pin="SDA" pad="35"/>
<connect gate="G$1" pin="USBD+" pad="42"/>
<connect gate="G$1" pin="USBD-" pad="41"/>
<connect gate="G$1" pin="VCC3.3@1" pad="11"/>
<connect gate="G$1" pin="VCC3.3@2" pad="22"/>
<connect gate="G$1" pin="VCC3.3@3" pad="33"/>
<connect gate="G$1" pin="VCC3.3@4" pad="44"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT" pad="9"/>
</connects>
<technologies>
<technology name="25">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="26">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="35">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EZ-USB-2122T" prefix="IC">
<description>Microcontroller with USB port</description>
<gates>
<gate name="G$1" symbol="EZ-USB-2122T"/>
</gates>
<devices>
<device name="" package="TQFP48_7X7">
<connects>
<connect gate="G$1" pin="!DISCON" pad="47"/>
<connect gate="G$1" pin="!WAKEUP" pad="40"/>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="AVCC" pad="11"/>
<connect gate="G$1" pin="BKPT" pad="35"/>
<connect gate="G$1" pin="CLK24" pad="2"/>
<connect gate="G$1" pin="CPU12MHZ" pad="15"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND/TEST" pad="41"/>
<connect gate="G$1" pin="GND/TEST1" pad="3"/>
<connect gate="G$1" pin="GND/TEST2" pad="4"/>
<connect gate="G$1" pin="GND/TEST3" pad="5"/>
<connect gate="G$1" pin="GND/TEST4" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="37"/>
<connect gate="G$1" pin="PA0/T0OUT" pad="34"/>
<connect gate="G$1" pin="PA4/!FWR" pad="42"/>
<connect gate="G$1" pin="PA5/!FRD" pad="43"/>
<connect gate="G$1" pin="PA6/RXD0OUT" pad="44"/>
<connect gate="G$1" pin="PA7/RXD1OUT" pad="8"/>
<connect gate="G$1" pin="PB0/T2" pad="26"/>
<connect gate="G$1" pin="PB1/T2EX" pad="27"/>
<connect gate="G$1" pin="PB2/RXD1" pad="28"/>
<connect gate="G$1" pin="PB3/TXD1" pad="29"/>
<connect gate="G$1" pin="PB4/INT4" pad="30"/>
<connect gate="G$1" pin="PB5/!INT5" pad="31"/>
<connect gate="G$1" pin="PB6/INT6" pad="32"/>
<connect gate="G$1" pin="PB7/T2OUT" pad="33"/>
<connect gate="G$1" pin="PC0/RXD0" pad="16"/>
<connect gate="G$1" pin="PC1/TXD0" pad="17"/>
<connect gate="G$1" pin="PC2/!INT0" pad="18"/>
<connect gate="G$1" pin="PC3/!INT1" pad="19"/>
<connect gate="G$1" pin="PC4/T0" pad="20"/>
<connect gate="G$1" pin="PC5/T1" pad="21"/>
<connect gate="G$1" pin="PC6/!WR" pad="22"/>
<connect gate="G$1" pin="PC7/!RD" pad="23"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="SCL" pad="39"/>
<connect gate="G$1" pin="SDA" pad="38"/>
<connect gate="G$1" pin="USBD+" pad="46"/>
<connect gate="G$1" pin="USBD-" pad="45"/>
<connect gate="G$1" pin="VCC3.3@1" pad="12"/>
<connect gate="G$1" pin="VCC3.3@2" pad="24"/>
<connect gate="G$1" pin="VCC3.3@3" pad="36"/>
<connect gate="G$1" pin="VCC3.3@4" pad="48"/>
<connect gate="G$1" pin="XIN" pad="9"/>
<connect gate="G$1" pin="XOUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EZ-USB-2126T" prefix="IC">
<description>Microcontroller with USB port</description>
<gates>
<gate name="G$1" symbol="EZ-USB-2126T"/>
</gates>
<devices>
<device name="" package="TQFP48_7X7">
<connects>
<connect gate="G$1" pin="!DISCON" pad="47"/>
<connect gate="G$1" pin="!WAKEUP" pad="40"/>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="AVCC" pad="11"/>
<connect gate="G$1" pin="BKPT" pad="35"/>
<connect gate="G$1" pin="CLK24" pad="2"/>
<connect gate="G$1" pin="CPU12MHZ" pad="15"/>
<connect gate="G$1" pin="D0" pad="26"/>
<connect gate="G$1" pin="D1" pad="27"/>
<connect gate="G$1" pin="D2" pad="28"/>
<connect gate="G$1" pin="D3" pad="29"/>
<connect gate="G$1" pin="D4" pad="30"/>
<connect gate="G$1" pin="D5" pad="31"/>
<connect gate="G$1" pin="D6" pad="32"/>
<connect gate="G$1" pin="D7" pad="33"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND/TEST" pad="41"/>
<connect gate="G$1" pin="GND/TEST1" pad="3"/>
<connect gate="G$1" pin="GND/TEST2" pad="4"/>
<connect gate="G$1" pin="GND/TEST3" pad="5"/>
<connect gate="G$1" pin="GND/TEST4" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="13"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="GND@3" pad="37"/>
<connect gate="G$1" pin="PA0/T0OUT" pad="34"/>
<connect gate="G$1" pin="PA4/!FWR" pad="42"/>
<connect gate="G$1" pin="PA5/!FRD" pad="43"/>
<connect gate="G$1" pin="PA6/RXD0OUT" pad="44"/>
<connect gate="G$1" pin="PA7/RXD1OUT" pad="8"/>
<connect gate="G$1" pin="PC0/RXD0" pad="16"/>
<connect gate="G$1" pin="PC1/TXD0" pad="17"/>
<connect gate="G$1" pin="PC2/!INT0" pad="18"/>
<connect gate="G$1" pin="PC3/!INT1" pad="19"/>
<connect gate="G$1" pin="PC4/T0" pad="20"/>
<connect gate="G$1" pin="PC5/T1" pad="21"/>
<connect gate="G$1" pin="PC6/!WR" pad="22"/>
<connect gate="G$1" pin="PC7/!RD" pad="23"/>
<connect gate="G$1" pin="RESET" pad="14"/>
<connect gate="G$1" pin="SCL" pad="39"/>
<connect gate="G$1" pin="SDA" pad="38"/>
<connect gate="G$1" pin="USBD+" pad="46"/>
<connect gate="G$1" pin="USBD-" pad="45"/>
<connect gate="G$1" pin="VCC3.3@1" pad="12"/>
<connect gate="G$1" pin="VCC3.3@2" pad="24"/>
<connect gate="G$1" pin="VCC3.3@3" pad="36"/>
<connect gate="G$1" pin="VCC3.3@4" pad="48"/>
<connect gate="G$1" pin="XIN" pad="9"/>
<connect gate="G$1" pin="XOUT" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CYWUSB6934" prefix="IC">
<description>&lt;b&gt;WirelessUSB LS 2.4 GHz DSSS Radio SoC&lt;/b&gt;&lt;p&gt;
Source: http://v4.cypress.com/cfuploads/img/products/cywusb6934.pdf</description>
<gates>
<gate name="G$1" symbol="CYWUSB6934"/>
</gates>
<devices>
<device name="-48LFG" package="QFN48">
<connects>
<connect gate="G$1" pin="!PD" pad="33"/>
<connect gate="G$1" pin="!RESET" pad="14"/>
<connect gate="G$1" pin="!SS" pad="22"/>
<connect gate="G$1" pin="DIO" pad="20"/>
<connect gate="G$1" pin="DIOVAL" pad="19"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="IRQ" pad="21"/>
<connect gate="G$1" pin="MISO" pad="24"/>
<connect gate="G$1" pin="MOSI" pad="23"/>
<connect gate="G$1" pin="PACTL" pad="34"/>
<connect gate="G$1" pin="RFIN" pad="46"/>
<connect gate="G$1" pin="RFOUT" pad="5"/>
<connect gate="G$1" pin="SCK" pad="25"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VCC@1" pad="9"/>
<connect gate="G$1" pin="VCC@2" pad="16"/>
<connect gate="G$1" pin="VCC@3" pad="28"/>
<connect gate="G$1" pin="VCC@4" pad="29"/>
<connect gate="G$1" pin="VCC@5" pad="32"/>
<connect gate="G$1" pin="VCC@6" pad="41"/>
<connect gate="G$1" pin="VCC@7" pad="42"/>
<connect gate="G$1" pin="VCC@8" pad="44"/>
<connect gate="G$1" pin="VCC@9" pad="45"/>
<connect gate="G$1" pin="X13" pad="38"/>
<connect gate="G$1" pin="X13IN" pad="35"/>
<connect gate="G$1" pin="X13OUT" pad="26"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-SE28" package="SOIC28-EPAD">
<connects>
<connect gate="G$1" pin="!PD" pad="23"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="!SS" pad="15"/>
<connect gate="G$1" pin="DIO" pad="13"/>
<connect gate="G$1" pin="DIOVAL" pad="12"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="IRQ" pad="14"/>
<connect gate="G$1" pin="MISO" pad="17"/>
<connect gate="G$1" pin="MOSI" pad="16"/>
<connect gate="G$1" pin="PACTL" pad="24"/>
<connect gate="G$1" pin="RFIN" pad="3"/>
<connect gate="G$1" pin="RFOUT" pad="6"/>
<connect gate="G$1" pin="SCK" pad="18"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VCC@1" pad="2"/>
<connect gate="G$1" pin="VCC@2" pad="7"/>
<connect gate="G$1" pin="VCC@3" pad="8"/>
<connect gate="G$1" pin="VCC@4" pad="11"/>
<connect gate="G$1" pin="VCC@5" pad="20"/>
<connect gate="G$1" pin="VCC@6" pad="21"/>
<connect gate="G$1" pin="VCC@7" pad="22"/>
<connect gate="G$1" pin="VCC@8" pad="27"/>
<connect gate="G$1" pin="VCC@9" pad="28"/>
<connect gate="G$1" pin="X13" pad="26"/>
<connect gate="G$1" pin="X13IN" pad="25"/>
<connect gate="G$1" pin="X13OUT" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CYWUSB6932" prefix="IC">
<description>&lt;b&gt;WirelessUSB LS 2.4 GHz DSSS Radio SoC&lt;/b&gt;&lt;p&gt;
Source: http://v4.cypress.com/cfuploads/img/products/cywusb6934.pdf</description>
<gates>
<gate name="G$1" symbol="CYWUSB6932"/>
</gates>
<devices>
<device name="-SE28" package="SOIC28-EPAD">
<connects>
<connect gate="G$1" pin="!PD" pad="23"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="!SS" pad="15"/>
<connect gate="G$1" pin="DIO" pad="13"/>
<connect gate="G$1" pin="DIOVAL" pad="12"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="GND@EXP" pad="EXP"/>
<connect gate="G$1" pin="IRQ" pad="14"/>
<connect gate="G$1" pin="MISO" pad="17"/>
<connect gate="G$1" pin="MOSI" pad="16"/>
<connect gate="G$1" pin="PACTL" pad="24"/>
<connect gate="G$1" pin="RFOUT" pad="6"/>
<connect gate="G$1" pin="SCK" pad="18"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VCC@1" pad="2"/>
<connect gate="G$1" pin="VCC@2" pad="7"/>
<connect gate="G$1" pin="VCC@3" pad="8"/>
<connect gate="G$1" pin="VCC@4" pad="11"/>
<connect gate="G$1" pin="VCC@5" pad="20"/>
<connect gate="G$1" pin="VCC@6" pad="21"/>
<connect gate="G$1" pin="VCC@7" pad="22"/>
<connect gate="G$1" pin="VCC@8" pad="27"/>
<connect gate="G$1" pin="VCC@9" pad="28"/>
<connect gate="G$1" pin="X13" pad="26"/>
<connect gate="G$1" pin="X13IN" pad="25"/>
<connect gate="G$1" pin="X13OUT" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C6801*A-128" prefix="IC">
<description>&lt;b&gt;EZ-USB FX2LP (TM) USB Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.cypress.com .. cy7c68013a_5.pdf</description>
<gates>
<gate name="G$1" symbol="CY7C68013A-128"/>
</gates>
<devices>
<device name="AXC" package="SQFP-R-14X20-128">
<connects>
<connect gate="G$1" pin="!CS" pad="42"/>
<connect gate="G$1" pin="!INT5" pad="106"/>
<connect gate="G$1" pin="!OE" pad="38"/>
<connect gate="G$1" pin="!PSEN" pad="39"/>
<connect gate="G$1" pin="!RD" pad="40"/>
<connect gate="G$1" pin="!RESET" pad="99"/>
<connect gate="G$1" pin="!WR" pad="41"/>
<connect gate="G$1" pin="A0" pad="94"/>
<connect gate="G$1" pin="A1" pad="95"/>
<connect gate="G$1" pin="A10" pad="128"/>
<connect gate="G$1" pin="A11" pad="21"/>
<connect gate="G$1" pin="A12" pad="22"/>
<connect gate="G$1" pin="A13" pad="23"/>
<connect gate="G$1" pin="A14" pad="24"/>
<connect gate="G$1" pin="A15" pad="25"/>
<connect gate="G$1" pin="A2" pad="96"/>
<connect gate="G$1" pin="A3" pad="97"/>
<connect gate="G$1" pin="A4" pad="117"/>
<connect gate="G$1" pin="A5" pad="118"/>
<connect gate="G$1" pin="A6" pad="119"/>
<connect gate="G$1" pin="A7" pad="120"/>
<connect gate="G$1" pin="A8" pad="126"/>
<connect gate="G$1" pin="A9" pad="127"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AGND@1" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="10"/>
<connect gate="G$1" pin="AVCC@1" pad="17"/>
<connect gate="G$1" pin="BKPT" pad="34"/>
<connect gate="G$1" pin="CLKOUT" pad="1"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="69"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="70"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="71"/>
<connect gate="G$1" pin="CTL3" pad="66"/>
<connect gate="G$1" pin="CTL4" pad="67"/>
<connect gate="G$1" pin="CTL5" pad="98"/>
<connect gate="G$1" pin="D0" pad="59"/>
<connect gate="G$1" pin="D1" pad="60"/>
<connect gate="G$1" pin="D2" pad="61"/>
<connect gate="G$1" pin="D3" pad="62"/>
<connect gate="G$1" pin="D4" pad="63"/>
<connect gate="G$1" pin="D5" pad="86"/>
<connect gate="G$1" pin="D6" pad="87"/>
<connect gate="G$1" pin="D7" pad="88"/>
<connect gate="G$1" pin="DMINUS" pad="19"/>
<connect gate="G$1" pin="DPLUS" pad="18"/>
<connect gate="G$1" pin="EA" pad="35"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="27"/>
<connect gate="G$1" pin="GND@2" pad="80"/>
<connect gate="G$1" pin="GND@3" pad="49"/>
<connect gate="G$1" pin="GND@4" pad="58"/>
<connect gate="G$1" pin="GND@5" pad="65"/>
<connect gate="G$1" pin="GND@6" pad="93"/>
<connect gate="G$1" pin="GND@7" pad="116"/>
<connect gate="G$1" pin="GND@8" pad="125"/>
<connect gate="G$1" pin="IFCLK" pad="32"/>
<connect gate="G$1" pin="INT4" pad="28"/>
<connect gate="G$1" pin="PA0/!INT0" pad="82"/>
<connect gate="G$1" pin="PA1/!INT1" pad="83"/>
<connect gate="G$1" pin="PA2/SLOE" pad="84"/>
<connect gate="G$1" pin="PA3/WU2" pad="85"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="89"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="90"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="91"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="92"/>
<connect gate="G$1" pin="PB0/FD0" pad="44"/>
<connect gate="G$1" pin="PB1/FD1" pad="45"/>
<connect gate="G$1" pin="PB2/FD2" pad="46"/>
<connect gate="G$1" pin="PB3/FD3" pad="47"/>
<connect gate="G$1" pin="PB4/FD4" pad="54"/>
<connect gate="G$1" pin="PB5/FD5" pad="55"/>
<connect gate="G$1" pin="PB6/FD6" pad="56"/>
<connect gate="G$1" pin="PB7/FD7" pad="57"/>
<connect gate="G$1" pin="PC0/GPIFADR0" pad="72"/>
<connect gate="G$1" pin="PC1/GPIFADR1" pad="73"/>
<connect gate="G$1" pin="PC2/GPIFADR2" pad="74"/>
<connect gate="G$1" pin="PC3/GPIFADR3" pad="75"/>
<connect gate="G$1" pin="PC4/GPIFADR4" pad="76"/>
<connect gate="G$1" pin="PC5/GPIFADR5" pad="77"/>
<connect gate="G$1" pin="PC6/GPIFADR6" pad="78"/>
<connect gate="G$1" pin="PC7/GPIFADR7" pad="79"/>
<connect gate="G$1" pin="PD0/FD8" pad="102"/>
<connect gate="G$1" pin="PD1/FD9" pad="103"/>
<connect gate="G$1" pin="PD2/FD10" pad="104"/>
<connect gate="G$1" pin="PD3/FD11" pad="105"/>
<connect gate="G$1" pin="PD4/FD12" pad="121"/>
<connect gate="G$1" pin="PD5/FD13" pad="122"/>
<connect gate="G$1" pin="PD6/FD14" pad="123"/>
<connect gate="G$1" pin="PD7/FD15" pad="124"/>
<connect gate="G$1" pin="PE0/T0OUT" pad="108"/>
<connect gate="G$1" pin="PE1/T1OUT" pad="109"/>
<connect gate="G$1" pin="PE2/T2OUT" pad="110"/>
<connect gate="G$1" pin="PE3/RXD0OUT" pad="111"/>
<connect gate="G$1" pin="PE4/RXD1OUT" pad="112"/>
<connect gate="G$1" pin="PE5/INT6" pad="113"/>
<connect gate="G$1" pin="PE6/T2EX" pad="114"/>
<connect gate="G$1" pin="PE7/GPIFADR8" pad="115"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="4"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="5"/>
<connect gate="G$1" pin="RDY2" pad="6"/>
<connect gate="G$1" pin="RDY3" pad="7"/>
<connect gate="G$1" pin="RDY4" pad="8"/>
<connect gate="G$1" pin="RDY5" pad="9"/>
<connect gate="G$1" pin="RESEVED" pad="33"/>
<connect gate="G$1" pin="RXD0" pad="51"/>
<connect gate="G$1" pin="RXD1" pad="53"/>
<connect gate="G$1" pin="SCL" pad="36"/>
<connect gate="G$1" pin="SDA" pad="37"/>
<connect gate="G$1" pin="T0" pad="29"/>
<connect gate="G$1" pin="T1" pad="30"/>
<connect gate="G$1" pin="T2" pad="31"/>
<connect gate="G$1" pin="TXD0" pad="50"/>
<connect gate="G$1" pin="TXD1" pad="52"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VCC@1" pad="26"/>
<connect gate="G$1" pin="VCC@2" pad="43"/>
<connect gate="G$1" pin="VCC@3" pad="48"/>
<connect gate="G$1" pin="VCC@4" pad="64"/>
<connect gate="G$1" pin="VCC@5" pad="68"/>
<connect gate="G$1" pin="VCC@6" pad="81"/>
<connect gate="G$1" pin="VCC@7" pad="100"/>
<connect gate="G$1" pin="VCC@8" pad="107"/>
<connect gate="G$1" pin="WAKEUP" pad="101"/>
<connect gate="G$1" pin="XTALIN" pad="12"/>
<connect gate="G$1" pin="XTALOUT" pad="11"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value="CYPRESS SEMICONDUCTOR CORPORAT"/>
<attribute name="MPN" value="CY7C68013A-128AXC"/>
<attribute name="OC_FARNELL" value="1269131"/>
<attribute name="OC_NEWARK" value="19M7108"/>
</technology>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C68014A-128AXC"/>
<attribute name="OC_FARNELL" value="1269137"/>
<attribute name="OC_NEWARK" value="23M5563"/>
</technology>
</technologies>
</device>
<device name="AXI" package="SQFP-R-14X20-128">
<connects>
<connect gate="G$1" pin="!CS" pad="42"/>
<connect gate="G$1" pin="!INT5" pad="106"/>
<connect gate="G$1" pin="!OE" pad="38"/>
<connect gate="G$1" pin="!PSEN" pad="39"/>
<connect gate="G$1" pin="!RD" pad="40"/>
<connect gate="G$1" pin="!RESET" pad="99"/>
<connect gate="G$1" pin="!WR" pad="41"/>
<connect gate="G$1" pin="A0" pad="94"/>
<connect gate="G$1" pin="A1" pad="95"/>
<connect gate="G$1" pin="A10" pad="128"/>
<connect gate="G$1" pin="A11" pad="21"/>
<connect gate="G$1" pin="A12" pad="22"/>
<connect gate="G$1" pin="A13" pad="23"/>
<connect gate="G$1" pin="A14" pad="24"/>
<connect gate="G$1" pin="A15" pad="25"/>
<connect gate="G$1" pin="A2" pad="96"/>
<connect gate="G$1" pin="A3" pad="97"/>
<connect gate="G$1" pin="A4" pad="117"/>
<connect gate="G$1" pin="A5" pad="118"/>
<connect gate="G$1" pin="A6" pad="119"/>
<connect gate="G$1" pin="A7" pad="120"/>
<connect gate="G$1" pin="A8" pad="126"/>
<connect gate="G$1" pin="A9" pad="127"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AGND@1" pad="20"/>
<connect gate="G$1" pin="AVCC" pad="10"/>
<connect gate="G$1" pin="AVCC@1" pad="17"/>
<connect gate="G$1" pin="BKPT" pad="34"/>
<connect gate="G$1" pin="CLKOUT" pad="1"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="69"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="70"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="71"/>
<connect gate="G$1" pin="CTL3" pad="66"/>
<connect gate="G$1" pin="CTL4" pad="67"/>
<connect gate="G$1" pin="CTL5" pad="98"/>
<connect gate="G$1" pin="D0" pad="59"/>
<connect gate="G$1" pin="D1" pad="60"/>
<connect gate="G$1" pin="D2" pad="61"/>
<connect gate="G$1" pin="D3" pad="62"/>
<connect gate="G$1" pin="D4" pad="63"/>
<connect gate="G$1" pin="D5" pad="86"/>
<connect gate="G$1" pin="D6" pad="87"/>
<connect gate="G$1" pin="D7" pad="88"/>
<connect gate="G$1" pin="DMINUS" pad="19"/>
<connect gate="G$1" pin="DPLUS" pad="18"/>
<connect gate="G$1" pin="EA" pad="35"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="27"/>
<connect gate="G$1" pin="GND@2" pad="80"/>
<connect gate="G$1" pin="GND@3" pad="49"/>
<connect gate="G$1" pin="GND@4" pad="58"/>
<connect gate="G$1" pin="GND@5" pad="65"/>
<connect gate="G$1" pin="GND@6" pad="93"/>
<connect gate="G$1" pin="GND@7" pad="116"/>
<connect gate="G$1" pin="GND@8" pad="125"/>
<connect gate="G$1" pin="IFCLK" pad="32"/>
<connect gate="G$1" pin="INT4" pad="28"/>
<connect gate="G$1" pin="PA0/!INT0" pad="82"/>
<connect gate="G$1" pin="PA1/!INT1" pad="83"/>
<connect gate="G$1" pin="PA2/SLOE" pad="84"/>
<connect gate="G$1" pin="PA3/WU2" pad="85"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="89"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="90"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="91"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="92"/>
<connect gate="G$1" pin="PB0/FD0" pad="44"/>
<connect gate="G$1" pin="PB1/FD1" pad="45"/>
<connect gate="G$1" pin="PB2/FD2" pad="46"/>
<connect gate="G$1" pin="PB3/FD3" pad="47"/>
<connect gate="G$1" pin="PB4/FD4" pad="54"/>
<connect gate="G$1" pin="PB5/FD5" pad="55"/>
<connect gate="G$1" pin="PB6/FD6" pad="56"/>
<connect gate="G$1" pin="PB7/FD7" pad="57"/>
<connect gate="G$1" pin="PC0/GPIFADR0" pad="72"/>
<connect gate="G$1" pin="PC1/GPIFADR1" pad="73"/>
<connect gate="G$1" pin="PC2/GPIFADR2" pad="74"/>
<connect gate="G$1" pin="PC3/GPIFADR3" pad="75"/>
<connect gate="G$1" pin="PC4/GPIFADR4" pad="76"/>
<connect gate="G$1" pin="PC5/GPIFADR5" pad="77"/>
<connect gate="G$1" pin="PC6/GPIFADR6" pad="78"/>
<connect gate="G$1" pin="PC7/GPIFADR7" pad="79"/>
<connect gate="G$1" pin="PD0/FD8" pad="102"/>
<connect gate="G$1" pin="PD1/FD9" pad="103"/>
<connect gate="G$1" pin="PD2/FD10" pad="104"/>
<connect gate="G$1" pin="PD3/FD11" pad="105"/>
<connect gate="G$1" pin="PD4/FD12" pad="121"/>
<connect gate="G$1" pin="PD5/FD13" pad="122"/>
<connect gate="G$1" pin="PD6/FD14" pad="123"/>
<connect gate="G$1" pin="PD7/FD15" pad="124"/>
<connect gate="G$1" pin="PE0/T0OUT" pad="108"/>
<connect gate="G$1" pin="PE1/T1OUT" pad="109"/>
<connect gate="G$1" pin="PE2/T2OUT" pad="110"/>
<connect gate="G$1" pin="PE3/RXD0OUT" pad="111"/>
<connect gate="G$1" pin="PE4/RXD1OUT" pad="112"/>
<connect gate="G$1" pin="PE5/INT6" pad="113"/>
<connect gate="G$1" pin="PE6/T2EX" pad="114"/>
<connect gate="G$1" pin="PE7/GPIFADR8" pad="115"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="4"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="5"/>
<connect gate="G$1" pin="RDY2" pad="6"/>
<connect gate="G$1" pin="RDY3" pad="7"/>
<connect gate="G$1" pin="RDY4" pad="8"/>
<connect gate="G$1" pin="RDY5" pad="9"/>
<connect gate="G$1" pin="RESEVED" pad="33"/>
<connect gate="G$1" pin="RXD0" pad="51"/>
<connect gate="G$1" pin="RXD1" pad="53"/>
<connect gate="G$1" pin="SCL" pad="36"/>
<connect gate="G$1" pin="SDA" pad="37"/>
<connect gate="G$1" pin="T0" pad="29"/>
<connect gate="G$1" pin="T1" pad="30"/>
<connect gate="G$1" pin="T2" pad="31"/>
<connect gate="G$1" pin="TXD0" pad="50"/>
<connect gate="G$1" pin="TXD1" pad="52"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VCC@1" pad="26"/>
<connect gate="G$1" pin="VCC@2" pad="43"/>
<connect gate="G$1" pin="VCC@3" pad="48"/>
<connect gate="G$1" pin="VCC@4" pad="64"/>
<connect gate="G$1" pin="VCC@5" pad="68"/>
<connect gate="G$1" pin="VCC@6" pad="81"/>
<connect gate="G$1" pin="VCC@7" pad="100"/>
<connect gate="G$1" pin="VCC@8" pad="107"/>
<connect gate="G$1" pin="WAKEUP" pad="101"/>
<connect gate="G$1" pin="XTALIN" pad="12"/>
<connect gate="G$1" pin="XTALOUT" pad="11"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C68013A-128AXI"/>
<attribute name="OC_FARNELL" value="1761052"/>
<attribute name="OC_NEWARK" value="19M7109"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C6801*A-100" prefix="IC">
<description>&lt;b&gt;EZ-USB FX2LP (TM) USB Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.cypress.com .. cy7c68013a_5.pdf</description>
<gates>
<gate name="G$1" symbol="CY7C68013A-100"/>
</gates>
<devices>
<device name="AXC" package="SQFP-R-14X20-100">
<connects>
<connect gate="G$1" pin="!INT5" pad="84"/>
<connect gate="G$1" pin="!RD" pad="31"/>
<connect gate="G$1" pin="!RESET" pad="77"/>
<connect gate="G$1" pin="!WR" pad="32"/>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="AGND@1" pad="19"/>
<connect gate="G$1" pin="AVCC" pad="9"/>
<connect gate="G$1" pin="AVCC@1" pad="16"/>
<connect gate="G$1" pin="BKPT" pad="28"/>
<connect gate="G$1" pin="CLKOUT" pad="100"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="54"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="55"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="56"/>
<connect gate="G$1" pin="CTL3" pad="51"/>
<connect gate="G$1" pin="CTL4" pad="52"/>
<connect gate="G$1" pin="CTL5" pad="76"/>
<connect gate="G$1" pin="DMINUS" pad="18"/>
<connect gate="G$1" pin="DPLUS" pad="17"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="21"/>
<connect gate="G$1" pin="GND@2" pad="39"/>
<connect gate="G$1" pin="GND@3" pad="48"/>
<connect gate="G$1" pin="GND@4" pad="50"/>
<connect gate="G$1" pin="GND@5" pad="65"/>
<connect gate="G$1" pin="GND@6" pad="75"/>
<connect gate="G$1" pin="GND@7" pad="94"/>
<connect gate="G$1" pin="GND@8" pad="99"/>
<connect gate="G$1" pin="IFCLK" pad="26"/>
<connect gate="G$1" pin="INT4" pad="22"/>
<connect gate="G$1" pin="PA0/!INT0" pad="67"/>
<connect gate="G$1" pin="PA1/!INT1" pad="68"/>
<connect gate="G$1" pin="PA2/SLOE" pad="69"/>
<connect gate="G$1" pin="PA3/WU2" pad="70"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="71"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="72"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="73"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="74"/>
<connect gate="G$1" pin="PB0/FD0" pad="34"/>
<connect gate="G$1" pin="PB1/FD1" pad="35"/>
<connect gate="G$1" pin="PB2/FD2" pad="36"/>
<connect gate="G$1" pin="PB3/FD3" pad="37"/>
<connect gate="G$1" pin="PB4/FD4" pad="44"/>
<connect gate="G$1" pin="PB5/FD5" pad="45"/>
<connect gate="G$1" pin="PB6/FD6" pad="46"/>
<connect gate="G$1" pin="PB7/FD7" pad="47"/>
<connect gate="G$1" pin="PC0/GPIFADR0" pad="57"/>
<connect gate="G$1" pin="PC1/GPIFADR1" pad="58"/>
<connect gate="G$1" pin="PC2/GPIFADR2" pad="59"/>
<connect gate="G$1" pin="PC3/GPIFADR3" pad="60"/>
<connect gate="G$1" pin="PC4/GPIFADR4" pad="61"/>
<connect gate="G$1" pin="PC5/GPIFADR5" pad="62"/>
<connect gate="G$1" pin="PC6/GPIFADR6" pad="63"/>
<connect gate="G$1" pin="PC7/GPIFADR7" pad="64"/>
<connect gate="G$1" pin="PD0/FD8" pad="80"/>
<connect gate="G$1" pin="PD1/FD9" pad="81"/>
<connect gate="G$1" pin="PD2/FD10" pad="82"/>
<connect gate="G$1" pin="PD3/FD11" pad="83"/>
<connect gate="G$1" pin="PD4/FD12" pad="95"/>
<connect gate="G$1" pin="PD5/FD13" pad="96"/>
<connect gate="G$1" pin="PD6/FD14" pad="97"/>
<connect gate="G$1" pin="PD7/FD15" pad="98"/>
<connect gate="G$1" pin="PE0/T0OUT" pad="86"/>
<connect gate="G$1" pin="PE1/T1OUT" pad="87"/>
<connect gate="G$1" pin="PE2/T2OUT" pad="88"/>
<connect gate="G$1" pin="PE3/RXD0OUT" pad="89"/>
<connect gate="G$1" pin="PE4/RXD1OUT" pad="90"/>
<connect gate="G$1" pin="PE5/INT6" pad="91"/>
<connect gate="G$1" pin="PE6/T2EX" pad="92"/>
<connect gate="G$1" pin="PE7/GPIFADR8" pad="93"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="3"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="4"/>
<connect gate="G$1" pin="RDY2" pad="5"/>
<connect gate="G$1" pin="RDY3" pad="6"/>
<connect gate="G$1" pin="RDY4" pad="7"/>
<connect gate="G$1" pin="RDY5" pad="8"/>
<connect gate="G$1" pin="RESEVED" pad="27"/>
<connect gate="G$1" pin="RXD0" pad="41"/>
<connect gate="G$1" pin="RXD1" pad="43"/>
<connect gate="G$1" pin="SCL" pad="29"/>
<connect gate="G$1" pin="SDA" pad="30"/>
<connect gate="G$1" pin="T0" pad="23"/>
<connect gate="G$1" pin="T1" pad="24"/>
<connect gate="G$1" pin="T2" pad="25"/>
<connect gate="G$1" pin="TXD0" pad="40"/>
<connect gate="G$1" pin="TXD1" pad="42"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VCC@1" pad="20"/>
<connect gate="G$1" pin="VCC@2" pad="33"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="VCC@4" pad="49"/>
<connect gate="G$1" pin="VCC@5" pad="66"/>
<connect gate="G$1" pin="VCC@6" pad="53"/>
<connect gate="G$1" pin="VCC@7" pad="78"/>
<connect gate="G$1" pin="VCC@8" pad="85"/>
<connect gate="G$1" pin="WAKEUP" pad="79"/>
<connect gate="G$1" pin="XTALIN" pad="11"/>
<connect gate="G$1" pin="XTALOUT" pad="10"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value="CYPRESS SEMICONDUCTOR CORPORAT"/>
<attribute name="MPN" value="CY7C68013A-100AXC"/>
<attribute name="OC_FARNELL" value="1269130"/>
<attribute name="OC_NEWARK" value="19M7106"/>
</technology>
<technology name="4">
<attribute name="MF" value="CYPRESS SEMICONDUCTOR CORPORAT"/>
<attribute name="MPN" value="CY7C68014A-100AXC"/>
<attribute name="OC_FARNELL" value="1269135"/>
<attribute name="OC_NEWARK" value="19M7117"/>
</technology>
</technologies>
</device>
<device name="AXI" package="SQFP-R-14X20-100">
<connects>
<connect gate="G$1" pin="!INT5" pad="84"/>
<connect gate="G$1" pin="!RD" pad="31"/>
<connect gate="G$1" pin="!RESET" pad="77"/>
<connect gate="G$1" pin="!WR" pad="32"/>
<connect gate="G$1" pin="AGND" pad="12"/>
<connect gate="G$1" pin="AGND@1" pad="19"/>
<connect gate="G$1" pin="AVCC" pad="9"/>
<connect gate="G$1" pin="AVCC@1" pad="16"/>
<connect gate="G$1" pin="BKPT" pad="28"/>
<connect gate="G$1" pin="CLKOUT" pad="100"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="54"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="55"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="56"/>
<connect gate="G$1" pin="CTL3" pad="51"/>
<connect gate="G$1" pin="CTL4" pad="52"/>
<connect gate="G$1" pin="CTL5" pad="76"/>
<connect gate="G$1" pin="DMINUS" pad="18"/>
<connect gate="G$1" pin="DPLUS" pad="17"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="21"/>
<connect gate="G$1" pin="GND@2" pad="39"/>
<connect gate="G$1" pin="GND@3" pad="48"/>
<connect gate="G$1" pin="GND@4" pad="50"/>
<connect gate="G$1" pin="GND@5" pad="65"/>
<connect gate="G$1" pin="GND@6" pad="75"/>
<connect gate="G$1" pin="GND@7" pad="94"/>
<connect gate="G$1" pin="GND@8" pad="99"/>
<connect gate="G$1" pin="IFCLK" pad="26"/>
<connect gate="G$1" pin="INT4" pad="22"/>
<connect gate="G$1" pin="PA0/!INT0" pad="67"/>
<connect gate="G$1" pin="PA1/!INT1" pad="68"/>
<connect gate="G$1" pin="PA2/SLOE" pad="69"/>
<connect gate="G$1" pin="PA3/WU2" pad="70"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="71"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="72"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="73"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="74"/>
<connect gate="G$1" pin="PB0/FD0" pad="34"/>
<connect gate="G$1" pin="PB1/FD1" pad="35"/>
<connect gate="G$1" pin="PB2/FD2" pad="36"/>
<connect gate="G$1" pin="PB3/FD3" pad="37"/>
<connect gate="G$1" pin="PB4/FD4" pad="44"/>
<connect gate="G$1" pin="PB5/FD5" pad="45"/>
<connect gate="G$1" pin="PB6/FD6" pad="46"/>
<connect gate="G$1" pin="PB7/FD7" pad="47"/>
<connect gate="G$1" pin="PC0/GPIFADR0" pad="57"/>
<connect gate="G$1" pin="PC1/GPIFADR1" pad="58"/>
<connect gate="G$1" pin="PC2/GPIFADR2" pad="59"/>
<connect gate="G$1" pin="PC3/GPIFADR3" pad="60"/>
<connect gate="G$1" pin="PC4/GPIFADR4" pad="61"/>
<connect gate="G$1" pin="PC5/GPIFADR5" pad="62"/>
<connect gate="G$1" pin="PC6/GPIFADR6" pad="63"/>
<connect gate="G$1" pin="PC7/GPIFADR7" pad="64"/>
<connect gate="G$1" pin="PD0/FD8" pad="80"/>
<connect gate="G$1" pin="PD1/FD9" pad="81"/>
<connect gate="G$1" pin="PD2/FD10" pad="82"/>
<connect gate="G$1" pin="PD3/FD11" pad="83"/>
<connect gate="G$1" pin="PD4/FD12" pad="95"/>
<connect gate="G$1" pin="PD5/FD13" pad="96"/>
<connect gate="G$1" pin="PD6/FD14" pad="97"/>
<connect gate="G$1" pin="PD7/FD15" pad="98"/>
<connect gate="G$1" pin="PE0/T0OUT" pad="86"/>
<connect gate="G$1" pin="PE1/T1OUT" pad="87"/>
<connect gate="G$1" pin="PE2/T2OUT" pad="88"/>
<connect gate="G$1" pin="PE3/RXD0OUT" pad="89"/>
<connect gate="G$1" pin="PE4/RXD1OUT" pad="90"/>
<connect gate="G$1" pin="PE5/INT6" pad="91"/>
<connect gate="G$1" pin="PE6/T2EX" pad="92"/>
<connect gate="G$1" pin="PE7/GPIFADR8" pad="93"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="3"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="4"/>
<connect gate="G$1" pin="RDY2" pad="5"/>
<connect gate="G$1" pin="RDY3" pad="6"/>
<connect gate="G$1" pin="RDY4" pad="7"/>
<connect gate="G$1" pin="RDY5" pad="8"/>
<connect gate="G$1" pin="RESEVED" pad="27"/>
<connect gate="G$1" pin="RXD0" pad="41"/>
<connect gate="G$1" pin="RXD1" pad="43"/>
<connect gate="G$1" pin="SCL" pad="29"/>
<connect gate="G$1" pin="SDA" pad="30"/>
<connect gate="G$1" pin="T0" pad="23"/>
<connect gate="G$1" pin="T1" pad="24"/>
<connect gate="G$1" pin="T2" pad="25"/>
<connect gate="G$1" pin="TXD0" pad="40"/>
<connect gate="G$1" pin="TXD1" pad="42"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VCC@1" pad="20"/>
<connect gate="G$1" pin="VCC@2" pad="33"/>
<connect gate="G$1" pin="VCC@3" pad="38"/>
<connect gate="G$1" pin="VCC@4" pad="49"/>
<connect gate="G$1" pin="VCC@5" pad="66"/>
<connect gate="G$1" pin="VCC@6" pad="53"/>
<connect gate="G$1" pin="VCC@7" pad="78"/>
<connect gate="G$1" pin="VCC@8" pad="85"/>
<connect gate="G$1" pin="WAKEUP" pad="79"/>
<connect gate="G$1" pin="XTALIN" pad="11"/>
<connect gate="G$1" pin="XTALOUT" pad="10"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C68013A-100AXI"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="19M7107"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C6801*A-56" prefix="IC">
<description>&lt;b&gt;EZ-USB FX2LP (TM) USB Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.cypress.com .. cy7c68013a_5.pdf</description>
<gates>
<gate name="G$1" symbol="CY7C68013A-56"/>
</gates>
<devices>
<device name="PVXC" package="SSOP56">
<connects>
<connect gate="G$1" pin="!RESET" pad="49"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AGND@1" pad="17"/>
<connect gate="G$1" pin="AVCC" pad="10"/>
<connect gate="G$1" pin="AVCC@1" pad="14"/>
<connect gate="G$1" pin="CLKOUT/T1OUT" pad="5"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="36"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="37"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="38"/>
<connect gate="G$1" pin="DMINUS" pad="16"/>
<connect gate="G$1" pin="DPLUS" pad="15"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="33"/>
<connect gate="G$1" pin="GND@4" pad="35"/>
<connect gate="G$1" pin="GND@5" pad="48"/>
<connect gate="G$1" pin="IFCLK/T0OUT" pad="20"/>
<connect gate="G$1" pin="PA0/!INT0" pad="40"/>
<connect gate="G$1" pin="PA1/!INT1" pad="41"/>
<connect gate="G$1" pin="PA2/SLOE" pad="42"/>
<connect gate="G$1" pin="PA3/WU2" pad="43"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="44"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="45"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="46"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="47"/>
<connect gate="G$1" pin="PB0/FD0" pad="25"/>
<connect gate="G$1" pin="PB1/FD1" pad="26"/>
<connect gate="G$1" pin="PB2/FD2" pad="27"/>
<connect gate="G$1" pin="PB3/FD3" pad="28"/>
<connect gate="G$1" pin="PB4/FD4" pad="29"/>
<connect gate="G$1" pin="PB5/FD5" pad="30"/>
<connect gate="G$1" pin="PB6/FD6" pad="31"/>
<connect gate="G$1" pin="PB7/FD7" pad="32"/>
<connect gate="G$1" pin="PD0/FD8" pad="52"/>
<connect gate="G$1" pin="PD1/FD9" pad="53"/>
<connect gate="G$1" pin="PD2/FD10" pad="54"/>
<connect gate="G$1" pin="PD3/FD11" pad="55"/>
<connect gate="G$1" pin="PD4/FD12" pad="56"/>
<connect gate="G$1" pin="PD5/FD13" pad="1"/>
<connect gate="G$1" pin="PD6/FD14" pad="2"/>
<connect gate="G$1" pin="PD7/FD15" pad="3"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="8"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="9"/>
<connect gate="G$1" pin="RESEVED" pad="21"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VCC@1" pad="18"/>
<connect gate="G$1" pin="VCC@2" pad="24"/>
<connect gate="G$1" pin="VCC@3" pad="34"/>
<connect gate="G$1" pin="VCC@4" pad="39"/>
<connect gate="G$1" pin="VCC@5" pad="50"/>
<connect gate="G$1" pin="WAKEUP" pad="51"/>
<connect gate="G$1" pin="XTALIN" pad="12"/>
<connect gate="G$1" pin="XTALOUT" pad="11"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value="CYPRESS SEMICONDUCTOR CORPORAT"/>
<attribute name="MPN" value="CY7C68013A-56PVXC"/>
<attribute name="OC_FARNELL" value="1269134"/>
<attribute name="OC_NEWARK" value="19M7114"/>
</technology>
<technology name="4">
<attribute name="MF" value="CYPRESS SEMICONDUCTOR CORPORAT"/>
<attribute name="MPN" value="CY7C68014A-56PVXC"/>
<attribute name="OC_FARNELL" value="1269140"/>
<attribute name="OC_NEWARK" value="19M7121"/>
</technology>
</technologies>
</device>
<device name="BAXC" package="VFBGA56">
<connects>
<connect gate="G$1" pin="!RESET" pad="B8"/>
<connect gate="G$1" pin="AGND" pad="F2"/>
<connect gate="G$1" pin="AGND@1" pad="F1"/>
<connect gate="G$1" pin="AVCC" pad="D2"/>
<connect gate="G$1" pin="AVCC@1" pad="D1"/>
<connect gate="G$1" pin="CLKOUT/T1OUT" pad="B2"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="H7"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="G7"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="H8"/>
<connect gate="G$1" pin="DMINUS" pad="E1"/>
<connect gate="G$1" pin="DPLUS" pad="E2"/>
<connect gate="G$1" pin="GND" pad="B4"/>
<connect gate="G$1" pin="GND@1" pad="H1"/>
<connect gate="G$1" pin="GND@2" pad="D7"/>
<connect gate="G$1" pin="GND@3" pad="D8"/>
<connect gate="G$1" pin="GND@4" pad="C4"/>
<connect gate="G$1" pin="GND@5" pad="A4"/>
<connect gate="G$1" pin="IFCLK/T0OUT" pad="G2"/>
<connect gate="G$1" pin="PA0/!INT0" pad="G8"/>
<connect gate="G$1" pin="PA1/!INT1" pad="G6"/>
<connect gate="G$1" pin="PA2/SLOE" pad="F8"/>
<connect gate="G$1" pin="PA3/WU2" pad="F7"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="F6"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="C8"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="C7"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="C6"/>
<connect gate="G$1" pin="PB0/FD0" pad="H3"/>
<connect gate="G$1" pin="PB1/FD1" pad="F4"/>
<connect gate="G$1" pin="PB2/FD2" pad="H4"/>
<connect gate="G$1" pin="PB3/FD3" pad="G4"/>
<connect gate="G$1" pin="PB4/FD4" pad="H5"/>
<connect gate="G$1" pin="PB5/FD5" pad="G5"/>
<connect gate="G$1" pin="PB6/FD6" pad="F5"/>
<connect gate="G$1" pin="PB7/FD7" pad="H6"/>
<connect gate="G$1" pin="PD0/FD8" pad="A8"/>
<connect gate="G$1" pin="PD1/FD9" pad="A7"/>
<connect gate="G$1" pin="PD2/FD10" pad="B6"/>
<connect gate="G$1" pin="PD3/FD11" pad="A6"/>
<connect gate="G$1" pin="PD4/FD12" pad="B3"/>
<connect gate="G$1" pin="PD5/FD13" pad="A3"/>
<connect gate="G$1" pin="PD6/FD14" pad="C3"/>
<connect gate="G$1" pin="PD7/FD15" pad="A2"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="A1"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="B1"/>
<connect gate="G$1" pin="RESEVED" pad="H2"/>
<connect gate="G$1" pin="SCL" pad="F3"/>
<connect gate="G$1" pin="SDA" pad="G3"/>
<connect gate="G$1" pin="VCC" pad="A5"/>
<connect gate="G$1" pin="VCC@1" pad="G1"/>
<connect gate="G$1" pin="VCC@2" pad="E7"/>
<connect gate="G$1" pin="VCC@3" pad="E8"/>
<connect gate="G$1" pin="VCC@4" pad="C5"/>
<connect gate="G$1" pin="VCC@5" pad="B5"/>
<connect gate="G$1" pin="WAKEUP" pad="B7"/>
<connect gate="G$1" pin="XTALIN" pad="C1"/>
<connect gate="G$1" pin="XTALOUT" pad="C2"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value="CYPRESS SEMICONDUCTOR CORPORAT"/>
<attribute name="MPN" value="CY7C68013A-56BAXC"/>
<attribute name="OC_FARNELL" value="1269132"/>
<attribute name="OC_NEWARK" value="19M7110"/>
</technology>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C68014A-56BAXC"/>
<attribute name="OC_FARNELL" value="1269138"/>
<attribute name="OC_NEWARK" value="23M5564"/>
</technology>
</technologies>
</device>
<device name="PVXI" package="SSOP56">
<connects>
<connect gate="G$1" pin="!RESET" pad="49"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AGND@1" pad="17"/>
<connect gate="G$1" pin="AVCC" pad="10"/>
<connect gate="G$1" pin="AVCC@1" pad="14"/>
<connect gate="G$1" pin="CLKOUT/T1OUT" pad="5"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="36"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="37"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="38"/>
<connect gate="G$1" pin="DMINUS" pad="16"/>
<connect gate="G$1" pin="DPLUS" pad="15"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="33"/>
<connect gate="G$1" pin="GND@4" pad="35"/>
<connect gate="G$1" pin="GND@5" pad="48"/>
<connect gate="G$1" pin="IFCLK/T0OUT" pad="20"/>
<connect gate="G$1" pin="PA0/!INT0" pad="40"/>
<connect gate="G$1" pin="PA1/!INT1" pad="41"/>
<connect gate="G$1" pin="PA2/SLOE" pad="42"/>
<connect gate="G$1" pin="PA3/WU2" pad="43"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="44"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="45"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="46"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="47"/>
<connect gate="G$1" pin="PB0/FD0" pad="25"/>
<connect gate="G$1" pin="PB1/FD1" pad="26"/>
<connect gate="G$1" pin="PB2/FD2" pad="27"/>
<connect gate="G$1" pin="PB3/FD3" pad="28"/>
<connect gate="G$1" pin="PB4/FD4" pad="29"/>
<connect gate="G$1" pin="PB5/FD5" pad="30"/>
<connect gate="G$1" pin="PB6/FD6" pad="31"/>
<connect gate="G$1" pin="PB7/FD7" pad="32"/>
<connect gate="G$1" pin="PD0/FD8" pad="52"/>
<connect gate="G$1" pin="PD1/FD9" pad="53"/>
<connect gate="G$1" pin="PD2/FD10" pad="54"/>
<connect gate="G$1" pin="PD3/FD11" pad="55"/>
<connect gate="G$1" pin="PD4/FD12" pad="56"/>
<connect gate="G$1" pin="PD5/FD13" pad="1"/>
<connect gate="G$1" pin="PD6/FD14" pad="2"/>
<connect gate="G$1" pin="PD7/FD15" pad="3"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="8"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="9"/>
<connect gate="G$1" pin="RESEVED" pad="21"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VCC@1" pad="18"/>
<connect gate="G$1" pin="VCC@2" pad="24"/>
<connect gate="G$1" pin="VCC@3" pad="34"/>
<connect gate="G$1" pin="VCC@4" pad="39"/>
<connect gate="G$1" pin="VCC@5" pad="50"/>
<connect gate="G$1" pin="WAKEUP" pad="51"/>
<connect gate="G$1" pin="XTALIN" pad="12"/>
<connect gate="G$1" pin="XTALOUT" pad="11"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C68013A-56PVXI"/>
<attribute name="OC_FARNELL" value="1761053"/>
<attribute name="OC_NEWARK" value="19M7116"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C6801*A-56QFN" prefix="IC">
<description>&lt;b&gt;EZ-USB FX2LP (TM) USB Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.cypress.com .. cy7c68013a_5.pdf</description>
<gates>
<gate name="G$1" symbol="CY7C68013A-56QFN"/>
</gates>
<devices>
<device name="LFXC" package="QFN56">
<connects>
<connect gate="G$1" pin="!RESET" pad="42"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AGND@1" pad="10"/>
<connect gate="G$1" pin="AVCC" pad="3"/>
<connect gate="G$1" pin="AVCC@1" pad="7"/>
<connect gate="G$1" pin="CLKOUT/T1OUT" pad="54"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="29"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="30"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="31"/>
<connect gate="G$1" pin="DMINUS" pad="9"/>
<connect gate="G$1" pin="DPLUS" pad="8"/>
<connect gate="G$1" pin="EPAD" pad="EPAD"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="26"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="41"/>
<connect gate="G$1" pin="GND@4" pad="53"/>
<connect gate="G$1" pin="GND@5" pad="56"/>
<connect gate="G$1" pin="IFCLK/T0OUT" pad="13"/>
<connect gate="G$1" pin="PA0/!INT0" pad="33"/>
<connect gate="G$1" pin="PA1/!INT1" pad="34"/>
<connect gate="G$1" pin="PA2/SLOE" pad="35"/>
<connect gate="G$1" pin="PA3/WU2" pad="36"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="37"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="38"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="39"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="40"/>
<connect gate="G$1" pin="PB0/FD0" pad="18"/>
<connect gate="G$1" pin="PB1/FD1" pad="19"/>
<connect gate="G$1" pin="PB2/FD2" pad="20"/>
<connect gate="G$1" pin="PB3/FD3" pad="21"/>
<connect gate="G$1" pin="PB4/FD4" pad="22"/>
<connect gate="G$1" pin="PB5/FD5" pad="23"/>
<connect gate="G$1" pin="PB6/FD6" pad="24"/>
<connect gate="G$1" pin="PB7/FD7" pad="25"/>
<connect gate="G$1" pin="PD0/FD8" pad="45"/>
<connect gate="G$1" pin="PD1/FD9" pad="46"/>
<connect gate="G$1" pin="PD2/FD10" pad="47"/>
<connect gate="G$1" pin="PD3/FD11" pad="48"/>
<connect gate="G$1" pin="PD4/FD12" pad="49"/>
<connect gate="G$1" pin="PD5/FD13" pad="50"/>
<connect gate="G$1" pin="PD6/FD14" pad="51"/>
<connect gate="G$1" pin="PD7/FD15" pad="52"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="1"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="2"/>
<connect gate="G$1" pin="RESEVED" pad="14"/>
<connect gate="G$1" pin="SCL" pad="15"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="17"/>
<connect gate="G$1" pin="VCC@2" pad="27"/>
<connect gate="G$1" pin="VCC@3" pad="32"/>
<connect gate="G$1" pin="VCC@4" pad="43"/>
<connect gate="G$1" pin="VCC@5" pad="55"/>
<connect gate="G$1" pin="WAKEUP" pad="44"/>
<connect gate="G$1" pin="XTALIN" pad="5"/>
<connect gate="G$1" pin="XTALOUT" pad="4"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="LFXI" package="QFN56">
<connects>
<connect gate="G$1" pin="!RESET" pad="42"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AGND@1" pad="10"/>
<connect gate="G$1" pin="AVCC" pad="3"/>
<connect gate="G$1" pin="AVCC@1" pad="7"/>
<connect gate="G$1" pin="CLKOUT/T1OUT" pad="54"/>
<connect gate="G$1" pin="CTL0/FLAGA" pad="29"/>
<connect gate="G$1" pin="CTL1/FLAGB" pad="30"/>
<connect gate="G$1" pin="CTL2/FLAGC" pad="31"/>
<connect gate="G$1" pin="DMINUS" pad="9"/>
<connect gate="G$1" pin="DPLUS" pad="8"/>
<connect gate="G$1" pin="EPAD" pad="EPAD"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="GND@1" pad="26"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="GND@3" pad="41"/>
<connect gate="G$1" pin="GND@4" pad="53"/>
<connect gate="G$1" pin="GND@5" pad="56"/>
<connect gate="G$1" pin="IFCLK/T0OUT" pad="13"/>
<connect gate="G$1" pin="PA0/!INT0" pad="33"/>
<connect gate="G$1" pin="PA1/!INT1" pad="34"/>
<connect gate="G$1" pin="PA2/SLOE" pad="35"/>
<connect gate="G$1" pin="PA3/WU2" pad="36"/>
<connect gate="G$1" pin="PA4/FIFOADR0" pad="37"/>
<connect gate="G$1" pin="PA5/FIFOADR1" pad="38"/>
<connect gate="G$1" pin="PA6/PKTEND" pad="39"/>
<connect gate="G$1" pin="PA7/FLAGD/!SLCS" pad="40"/>
<connect gate="G$1" pin="PB0/FD0" pad="18"/>
<connect gate="G$1" pin="PB1/FD1" pad="19"/>
<connect gate="G$1" pin="PB2/FD2" pad="20"/>
<connect gate="G$1" pin="PB3/FD3" pad="21"/>
<connect gate="G$1" pin="PB4/FD4" pad="22"/>
<connect gate="G$1" pin="PB5/FD5" pad="23"/>
<connect gate="G$1" pin="PB6/FD6" pad="24"/>
<connect gate="G$1" pin="PB7/FD7" pad="25"/>
<connect gate="G$1" pin="PD0/FD8" pad="45"/>
<connect gate="G$1" pin="PD1/FD9" pad="46"/>
<connect gate="G$1" pin="PD2/FD10" pad="47"/>
<connect gate="G$1" pin="PD3/FD11" pad="48"/>
<connect gate="G$1" pin="PD4/FD12" pad="49"/>
<connect gate="G$1" pin="PD5/FD13" pad="50"/>
<connect gate="G$1" pin="PD6/FD14" pad="51"/>
<connect gate="G$1" pin="PD7/FD15" pad="52"/>
<connect gate="G$1" pin="RDY0/SLRD" pad="1"/>
<connect gate="G$1" pin="RDY1/SLRW" pad="2"/>
<connect gate="G$1" pin="RESEVED" pad="14"/>
<connect gate="G$1" pin="SCL" pad="15"/>
<connect gate="G$1" pin="SDA" pad="16"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC@1" pad="17"/>
<connect gate="G$1" pin="VCC@2" pad="27"/>
<connect gate="G$1" pin="VCC@3" pad="32"/>
<connect gate="G$1" pin="VCC@4" pad="43"/>
<connect gate="G$1" pin="VCC@5" pad="55"/>
<connect gate="G$1" pin="WAKEUP" pad="44"/>
<connect gate="G$1" pin="XTALIN" pad="5"/>
<connect gate="G$1" pin="XTALOUT" pad="4"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C63001C-?XC*" prefix="IC">
<description>&lt;b&gt;Universal Serial Bus Microcontroller&lt;/b&gt;&lt;p&gt;
Integrated USB transceiver&lt;br&gt;
Source: www.cypress.com .. CY7C6301XX.pdf</description>
<gates>
<gate name="G$1" symbol="CY7C63001"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="CEXT" pad="9"/>
<connect gate="G$1" pin="D+" pad="14"/>
<connect gate="G$1" pin="D-" pad="13"/>
<connect gate="G$1" pin="P0.0" pad="1"/>
<connect gate="G$1" pin="P0.1" pad="2"/>
<connect gate="G$1" pin="P0.2" pad="3"/>
<connect gate="G$1" pin="P0.3" pad="4"/>
<connect gate="G$1" pin="P0.4" pad="20"/>
<connect gate="G$1" pin="P0.5" pad="19"/>
<connect gate="G$1" pin="P0.6" pad="18"/>
<connect gate="G$1" pin="P0.7" pad="17"/>
<connect gate="G$1" pin="P1.0" pad="5"/>
<connect gate="G$1" pin="P1.1" pad="16"/>
<connect gate="G$1" pin="P1.2" pad="6"/>
<connect gate="G$1" pin="P1.3" pad="15"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VPP" pad="8"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="XTALIN" pad="10"/>
<connect gate="G$1" pin="XTALOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C63001C-PXC"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="19M7032"/>
</technology>
</technologies>
</device>
<device name="S" package="SO20L">
<connects>
<connect gate="G$1" pin="CEXT" pad="9"/>
<connect gate="G$1" pin="D+" pad="14"/>
<connect gate="G$1" pin="D-" pad="13"/>
<connect gate="G$1" pin="P0.0" pad="1"/>
<connect gate="G$1" pin="P0.1" pad="2"/>
<connect gate="G$1" pin="P0.2" pad="3"/>
<connect gate="G$1" pin="P0.3" pad="4"/>
<connect gate="G$1" pin="P0.4" pad="20"/>
<connect gate="G$1" pin="P0.5" pad="19"/>
<connect gate="G$1" pin="P0.6" pad="18"/>
<connect gate="G$1" pin="P0.7" pad="17"/>
<connect gate="G$1" pin="P1.0" pad="5"/>
<connect gate="G$1" pin="P1.1" pad="16"/>
<connect gate="G$1" pin="P1.2" pad="6"/>
<connect gate="G$1" pin="P1.3" pad="15"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VPP" pad="8"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="XTALIN" pad="10"/>
<connect gate="G$1" pin="XTALOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C63001C-SXC"/>
<attribute name="OC_FARNELL" value="1769872"/>
<attribute name="OC_NEWARK" value="19M7033"/>
</technology>
<technology name="T">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C63001C-SXCT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="19M7034"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C63101CQXC" prefix="IC">
<description>&lt;b&gt;Universal Serial Bus Microcontroller&lt;/b&gt;&lt;p&gt;
Integrated USB transceiver&lt;br&gt;
Source: www.cypress.com .. CY7C6301XX.pdf</description>
<gates>
<gate name="G$1" symbol="CY7C63101C-QXC"/>
</gates>
<devices>
<device name="" package="QSOP24">
<connects>
<connect gate="G$1" pin="CEXT" pad="11"/>
<connect gate="G$1" pin="D+" pad="16"/>
<connect gate="G$1" pin="D-" pad="15"/>
<connect gate="G$1" pin="P0.0" pad="1"/>
<connect gate="G$1" pin="P0.1" pad="2"/>
<connect gate="G$1" pin="P0.2" pad="3"/>
<connect gate="G$1" pin="P0.3" pad="4"/>
<connect gate="G$1" pin="P0.4" pad="24"/>
<connect gate="G$1" pin="P0.5" pad="23"/>
<connect gate="G$1" pin="P0.6" pad="22"/>
<connect gate="G$1" pin="P0.7" pad="21"/>
<connect gate="G$1" pin="P1.0" pad="5"/>
<connect gate="G$1" pin="P1.1" pad="20"/>
<connect gate="G$1" pin="P1.2" pad="6"/>
<connect gate="G$1" pin="P1.3" pad="19"/>
<connect gate="G$1" pin="P1.4" pad="7"/>
<connect gate="G$1" pin="P1.5" pad="18"/>
<connect gate="G$1" pin="P1.6" pad="8"/>
<connect gate="G$1" pin="P1.7" pad="17"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VPP" pad="10"/>
<connect gate="G$1" pin="VSS" pad="9"/>
<connect gate="G$1" pin="XTALIN" pad="12"/>
<connect gate="G$1" pin="XTALOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY7C63101C-QXC"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="19M7035"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C2*345" prefix="IC">
<description>&lt;b&gt;PSoC® Programmable System-on-Chip TM&lt;/b&gt;&lt;p&gt;
M8C Processor Speeds up to 24 MHz&lt;br&gt;
Source: http://www.cypress.com .. CY8C213452.pdf</description>
<gates>
<gate name="G$1" symbol="CY8C22345"/>
</gates>
<devices>
<device name="" package="SOIC28-3">
<connects>
<connect gate="G$1" pin="ADC_VREF/ML/P2[5]" pad="6"/>
<connect gate="G$1" pin="AI/ML/P0[1]" pad="4"/>
<connect gate="G$1" pin="AI/ML/P0[3]" pad="3"/>
<connect gate="G$1" pin="AI/ML/P0[5]" pad="2"/>
<connect gate="G$1" pin="AI/ML/P2[7]" pad="5"/>
<connect gate="G$1" pin="AI/MR/P0[7]" pad="1"/>
<connect gate="G$1" pin="I2C_SCL/ML/P1[1]" pad="13"/>
<connect gate="G$1" pin="I2C_SCL/ML/P1[7]" pad="10"/>
<connect gate="G$1" pin="I2C_SDA/ML/P1[5]" pad="11"/>
<connect gate="G$1" pin="ML/P1[3]" pad="12"/>
<connect gate="G$1" pin="ML/P2[1]" pad="8"/>
<connect gate="G$1" pin="ML/P2[3]" pad="7"/>
<connect gate="G$1" pin="P0[0]/MR/AI" pad="24"/>
<connect gate="G$1" pin="P0[2]/MR/AI" pad="25"/>
<connect gate="G$1" pin="P0[4]/MR/AI" pad="26"/>
<connect gate="G$1" pin="P0[6]/MR/AI" pad="27"/>
<connect gate="G$1" pin="P1[0]/MR/I2C_SDA" pad="15"/>
<connect gate="G$1" pin="P1[2]/MR" pad="16"/>
<connect gate="G$1" pin="P1[4]/MR/EXTCLK" pad="17"/>
<connect gate="G$1" pin="P1[6]/MR" pad="18"/>
<connect gate="G$1" pin="P2[0]/MR" pad="20"/>
<connect gate="G$1" pin="P2[2]/MR" pad="21"/>
<connect gate="G$1" pin="P2[4]/MR" pad="22"/>
<connect gate="G$1" pin="P2[6]/MR/AI" pad="23"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="14"/>
<connect gate="G$1" pin="XRES" pad="19"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY3250-22345"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="50R9266"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C22545" prefix="IC">
<description>&lt;b&gt;PSoC® Programmable System-on-Chip TM&lt;/b&gt;&lt;p&gt;
M8C Processor Speeds up to 24 MHz&lt;br&gt;
Source: http://www.cypress.com .. CY8C213452.pdf</description>
<gates>
<gate name="G$1" symbol="CY8C22545"/>
</gates>
<devices>
<device name="T" package="TQFP44">
<connects>
<connect gate="G$1" pin="ADC_VREF/ML/P2[5]" pad="1"/>
<connect gate="G$1" pin="AI/ML/P0[1]" pad="43"/>
<connect gate="G$1" pin="AI/ML/P0[3]" pad="42"/>
<connect gate="G$1" pin="AI/ML/P0[5]" pad="41"/>
<connect gate="G$1" pin="AI/ML/P2[7]" pad="44"/>
<connect gate="G$1" pin="AI/MR/P0[0]" pad="35"/>
<connect gate="G$1" pin="AI/MR/P0[2]" pad="36"/>
<connect gate="G$1" pin="AI/MR/P0[4]" pad="37"/>
<connect gate="G$1" pin="AI/MR/P0[6]" pad="38"/>
<connect gate="G$1" pin="AI/MR/P0[7]" pad="40"/>
<connect gate="G$1" pin="AI/MR/P2[6]" pad="34"/>
<connect gate="G$1" pin="EXTCLK/MR/P1[4]" pad="20"/>
<connect gate="G$1" pin="I2C_SCA/XTALOUT/MR/P1[0]" pad="18"/>
<connect gate="G$1" pin="I2C_SCL/ML/P1[7]" pad="13"/>
<connect gate="G$1" pin="I2C_SCL/XTALIN/ML/P1[1]" pad="16"/>
<connect gate="G$1" pin="I2C_SDA/ML/P1[5]" pad="14"/>
<connect gate="G$1" pin="ML/P1[3]" pad="15"/>
<connect gate="G$1" pin="ML/P2[1]" pad="3"/>
<connect gate="G$1" pin="ML/P2[3]" pad="2"/>
<connect gate="G$1" pin="ML/P3[1]" pad="12"/>
<connect gate="G$1" pin="ML/P3[3]" pad="11"/>
<connect gate="G$1" pin="ML/P3[5]" pad="10"/>
<connect gate="G$1" pin="ML/P3[7]" pad="9"/>
<connect gate="G$1" pin="ML/P4[1]" pad="7"/>
<connect gate="G$1" pin="ML/P4[3]" pad="6"/>
<connect gate="G$1" pin="ML/P4[5]" pad="5"/>
<connect gate="G$1" pin="MR/P1[2]" pad="19"/>
<connect gate="G$1" pin="MR/P1[6]" pad="21"/>
<connect gate="G$1" pin="MR/P2[0]" pad="31"/>
<connect gate="G$1" pin="MR/P2[2]" pad="32"/>
<connect gate="G$1" pin="MR/P2[4]" pad="33"/>
<connect gate="G$1" pin="MR/P3[0]" pad="22"/>
<connect gate="G$1" pin="MR/P3[2]" pad="23"/>
<connect gate="G$1" pin="MR/P3[4]" pad="24"/>
<connect gate="G$1" pin="MR/P3[6]" pad="25"/>
<connect gate="G$1" pin="MR/P4[0]" pad="27"/>
<connect gate="G$1" pin="MR/P4[2]" pad="28"/>
<connect gate="G$1" pin="MR/P4[4]" pad="29"/>
<connect gate="G$1" pin="VDD@1" pad="4"/>
<connect gate="G$1" pin="VDD@2" pad="39"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="17"/>
<connect gate="G$1" pin="VSS@3" pad="30"/>
<connect gate="G$1" pin="XRES" pad="26"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C21234" prefix="IC">
<description>&lt;b&gt;PSoC® Programmable System-on-Chip?&lt;/b&gt;&lt;p&gt;
M8C Processor Speeds to 24 MHz&lt;br&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
<gates>
<gate name="G$1" symbol="CY8C21234"/>
</gates>
<devices>
<device name="" package="SOIC16">
<connects>
<connect gate="G$1" pin="A/I/M/P0[1]" pad="4"/>
<connect gate="G$1" pin="A/I/M/P0[3]" pad="3"/>
<connect gate="G$1" pin="A/I/M/P0[5]" pad="2"/>
<connect gate="G$1" pin="A/I/M/P0[7]" pad="1"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[1]" pad="7"/>
<connect gate="G$1" pin="P0[0]/M/I/A" pad="12"/>
<connect gate="G$1" pin="P0[2]/M/I/A" pad="13"/>
<connect gate="G$1" pin="P0[4]/M/I/A" pad="14"/>
<connect gate="G$1" pin="P0[6]/M/I/A" pad="15"/>
<connect gate="G$1" pin="P1[0]/I2C_SDA/M" pad="9"/>
<connect gate="G$1" pin="P1[2]/M" pad="10"/>
<connect gate="G$1" pin="P1[4]/EXTCLK/M" pad="11"/>
<connect gate="G$1" pin="SMP" pad="5"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY8C21234-24SXI"/>
<attribute name="OC_FARNELL" value="1321728"/>
<attribute name="OC_NEWARK" value="19M7160"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C21334" prefix="IC">
<description>&lt;b&gt;PSoC® Programmable System-on-Chip?&lt;/b&gt;&lt;p&gt;
M8C Processor Speeds to 24 MHz&lt;br&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
<gates>
<gate name="G$1" symbol="CY8C21334"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="G$1" pin="A/I/M/P0[1]" pad="4"/>
<connect gate="G$1" pin="A/I/M/P0[3]" pad="3"/>
<connect gate="G$1" pin="A/I/M/P0[5]" pad="2"/>
<connect gate="G$1" pin="A/I/M/P0[7]" pad="1"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[1]" pad="9"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[7]" pad="6"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[5]" pad="7"/>
<connect gate="G$1" pin="MP1[3]" pad="8"/>
<connect gate="G$1" pin="P0[0]/M/I/A" pad="16"/>
<connect gate="G$1" pin="P0[2]/M/I/A" pad="17"/>
<connect gate="G$1" pin="P0[4]/M/I/A" pad="18"/>
<connect gate="G$1" pin="P0[6]/M/I/A" pad="19"/>
<connect gate="G$1" pin="P1[0]/I2C_SDA/M" pad="11"/>
<connect gate="G$1" pin="P1[2]/M" pad="12"/>
<connect gate="G$1" pin="P1[4]/EXT_CLK/M" pad="13"/>
<connect gate="G$1" pin="P1[6]/M" pad="14"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS@1" pad="5"/>
<connect gate="G$1" pin="VSS@2" pad="10"/>
<connect gate="G$1" pin="XRES" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY8C21334-12PVXE"/>
<attribute name="OC_FARNELL" value="1321731"/>
<attribute name="OC_NEWARK" value="53M3699"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C21534" prefix="IC">
<description>&lt;b&gt;PSoC® Programmable System-on-Chip?&lt;/b&gt;&lt;p&gt;
M8C Processor Speeds to 24 MHz&lt;br&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
<gates>
<gate name="G$1" symbol="CY8C21534"/>
</gates>
<devices>
<device name="" package="SSOP28">
<connects>
<connect gate="G$1" pin="A/I/M/P0[1]" pad="4"/>
<connect gate="G$1" pin="A/I/M/P0[3]" pad="3"/>
<connect gate="G$1" pin="A/I/M/P0[5]" pad="2"/>
<connect gate="G$1" pin="A/I/M/P0[7]" pad="1"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[1]" pad="13"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[7]" pad="10"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[5]" pad="11"/>
<connect gate="G$1" pin="M/P1[3]" pad="12"/>
<connect gate="G$1" pin="M/P2[1]" pad="8"/>
<connect gate="G$1" pin="M/P2[3]" pad="7"/>
<connect gate="G$1" pin="M/P2[5]" pad="6"/>
<connect gate="G$1" pin="M/P2[7]" pad="5"/>
<connect gate="G$1" pin="P0[0]/A/I/M" pad="24"/>
<connect gate="G$1" pin="P0[2]/A/I/M" pad="25"/>
<connect gate="G$1" pin="P0[4]/A/I/M" pad="26"/>
<connect gate="G$1" pin="P0[6]/A/I/M" pad="27"/>
<connect gate="G$1" pin="P1[0]/I2C_SDA/M" pad="15"/>
<connect gate="G$1" pin="P1[2]/M" pad="16"/>
<connect gate="G$1" pin="P1[4]/EXTCLK/M" pad="17"/>
<connect gate="G$1" pin="P1[6]/M" pad="18"/>
<connect gate="G$1" pin="P2[0]/M" pad="20"/>
<connect gate="G$1" pin="P2[2]/M" pad="21"/>
<connect gate="G$1" pin="P2[4]/M" pad="22"/>
<connect gate="G$1" pin="P2[6]/M" pad="23"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="9"/>
<connect gate="G$1" pin="VSS@2" pad="14"/>
<connect gate="G$1" pin="XRES" pad="19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CY8C21534-12PVXE"/>
<attribute name="OC_FARNELL" value="1321733"/>
<attribute name="OC_NEWARK" value="19M7172"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C21434" prefix="IC">
<description>&lt;b&gt;PSoC® Programmable System-on-Chip?&lt;/b&gt;&lt;p&gt;
M8C Processor Speeds to 24 MHz&lt;br&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
<gates>
<gate name="G$1" symbol="CY8C21434"/>
</gates>
<devices>
<device name="" package="QFN32">
<connects>
<connect gate="G$1" pin="A/I/M/P0[1]" pad="1"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="M/12C_SCL/P1[7]" pad="8"/>
<connect gate="G$1" pin="M/EXTCLK/P1[4]" pad="15"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[1]" pad="11"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[0]" pad="13"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[5]" pad="9"/>
<connect gate="G$1" pin="M/P1[2]" pad="14"/>
<connect gate="G$1" pin="M/P1[3]" pad="10"/>
<connect gate="G$1" pin="M/P1[6]" pad="16"/>
<connect gate="G$1" pin="M/P2[1]" pad="5"/>
<connect gate="G$1" pin="M/P2[3]" pad="4"/>
<connect gate="G$1" pin="M/P2[5]" pad="3"/>
<connect gate="G$1" pin="M/P2[7]" pad="2"/>
<connect gate="G$1" pin="M/P3[1]" pad="7"/>
<connect gate="G$1" pin="M/P3[3]" pad="6"/>
<connect gate="G$1" pin="P0[0]/A/I/M" pad="24"/>
<connect gate="G$1" pin="P0[2]/A/I/M" pad="25"/>
<connect gate="G$1" pin="P0[3]/A/I/M" pad="31"/>
<connect gate="G$1" pin="P0[4]/A/I/M" pad="26"/>
<connect gate="G$1" pin="P0[5]/A/I/M" pad="30"/>
<connect gate="G$1" pin="P0[6]/A/I/M" pad="27"/>
<connect gate="G$1" pin="P0[7]/A/I/M" pad="29"/>
<connect gate="G$1" pin="P2[0]/M" pad="20"/>
<connect gate="G$1" pin="P2[2]/M" pad="21"/>
<connect gate="G$1" pin="P2[4]/M" pad="22"/>
<connect gate="G$1" pin="P2[6]/M" pad="23"/>
<connect gate="G$1" pin="P3[0]/M" pad="18"/>
<connect gate="G$1" pin="P3[2]/M" pad="19"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
<connect gate="G$1" pin="VSS@2" pad="32"/>
<connect gate="G$1" pin="XRES" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1321732"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SAWN" package="QFN32-SAWN">
<connects>
<connect gate="G$1" pin="A/I/M/P0[1]" pad="1"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="M/12C_SCL/P1[7]" pad="8"/>
<connect gate="G$1" pin="M/EXTCLK/P1[4]" pad="15"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[1]" pad="11"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[0]" pad="13"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[5]" pad="9"/>
<connect gate="G$1" pin="M/P1[2]" pad="14"/>
<connect gate="G$1" pin="M/P1[3]" pad="10"/>
<connect gate="G$1" pin="M/P1[6]" pad="16"/>
<connect gate="G$1" pin="M/P2[1]" pad="5"/>
<connect gate="G$1" pin="M/P2[3]" pad="4"/>
<connect gate="G$1" pin="M/P2[5]" pad="3"/>
<connect gate="G$1" pin="M/P2[7]" pad="2"/>
<connect gate="G$1" pin="M/P3[1]" pad="7"/>
<connect gate="G$1" pin="M/P3[3]" pad="6"/>
<connect gate="G$1" pin="P0[0]/A/I/M" pad="24"/>
<connect gate="G$1" pin="P0[2]/A/I/M" pad="25"/>
<connect gate="G$1" pin="P0[3]/A/I/M" pad="31"/>
<connect gate="G$1" pin="P0[4]/A/I/M" pad="26"/>
<connect gate="G$1" pin="P0[5]/A/I/M" pad="30"/>
<connect gate="G$1" pin="P0[6]/A/I/M" pad="27"/>
<connect gate="G$1" pin="P0[7]/A/I/M" pad="29"/>
<connect gate="G$1" pin="P2[0]/M" pad="20"/>
<connect gate="G$1" pin="P2[2]/M" pad="21"/>
<connect gate="G$1" pin="P2[4]/M" pad="22"/>
<connect gate="G$1" pin="P2[6]/M" pad="23"/>
<connect gate="G$1" pin="P3[0]/M" pad="18"/>
<connect gate="G$1" pin="P3[2]/M" pad="19"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
<connect gate="G$1" pin="VSS@2" pad="32"/>
<connect gate="G$1" pin="XRES" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C21634" prefix="IC">
<description>&lt;b&gt;PSoC® Programmable System-on-Chip?&lt;/b&gt;&lt;p&gt;
M8C Processor Speeds to 24 MHz&lt;br&gt;
Source: http://www.cypress.com .. 38-12025_0P_V.pdf</description>
<gates>
<gate name="G$1" symbol="CY8C21634"/>
</gates>
<devices>
<device name="" package="QFN32">
<connects>
<connect gate="G$1" pin="A/I/M/P0[1]" pad="1"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="M/12C_SCL/P1[7]" pad="8"/>
<connect gate="G$1" pin="M/EXTCLK/P1[4]" pad="15"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[1]" pad="11"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[0]" pad="13"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[5]" pad="9"/>
<connect gate="G$1" pin="M/P1[2]" pad="14"/>
<connect gate="G$1" pin="M/P1[3]" pad="10"/>
<connect gate="G$1" pin="M/P1[6]" pad="16"/>
<connect gate="G$1" pin="M/P2[1]" pad="5"/>
<connect gate="G$1" pin="M/P2[3]" pad="4"/>
<connect gate="G$1" pin="M/P2[5]" pad="3"/>
<connect gate="G$1" pin="M/P2[7]" pad="2"/>
<connect gate="G$1" pin="P0[0]/A/I/M" pad="24"/>
<connect gate="G$1" pin="P0[2]/A/I/M" pad="25"/>
<connect gate="G$1" pin="P0[3]/A/I/M" pad="31"/>
<connect gate="G$1" pin="P0[4]/A/I/M" pad="26"/>
<connect gate="G$1" pin="P0[5]/A/I/M" pad="30"/>
<connect gate="G$1" pin="P0[6]/A/I/M" pad="27"/>
<connect gate="G$1" pin="P0[7]/A/I/M" pad="29"/>
<connect gate="G$1" pin="P2[0]/M" pad="20"/>
<connect gate="G$1" pin="P2[2]/M" pad="21"/>
<connect gate="G$1" pin="P2[4]/M" pad="22"/>
<connect gate="G$1" pin="P2[6]/M" pad="23"/>
<connect gate="G$1" pin="P3[0]/M" pad="18"/>
<connect gate="G$1" pin="P3[2]/M" pad="19"/>
<connect gate="G$1" pin="SMP" pad="6"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
<connect gate="G$1" pin="VSS@2" pad="32"/>
<connect gate="G$1" pin="XRES" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1321734"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SAWN" package="QFN32-SAWN">
<connects>
<connect gate="G$1" pin="A/I/M/P0[1]" pad="1"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="M/12C_SCL/P1[7]" pad="8"/>
<connect gate="G$1" pin="M/EXTCLK/P1[4]" pad="15"/>
<connect gate="G$1" pin="M/I2C_SCL/P1[1]" pad="11"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[0]" pad="13"/>
<connect gate="G$1" pin="M/I2C_SDA/P1[5]" pad="9"/>
<connect gate="G$1" pin="M/P1[2]" pad="14"/>
<connect gate="G$1" pin="M/P1[3]" pad="10"/>
<connect gate="G$1" pin="M/P1[6]" pad="16"/>
<connect gate="G$1" pin="M/P2[1]" pad="5"/>
<connect gate="G$1" pin="M/P2[3]" pad="4"/>
<connect gate="G$1" pin="M/P2[5]" pad="3"/>
<connect gate="G$1" pin="M/P2[7]" pad="2"/>
<connect gate="G$1" pin="P0[0]/A/I/M" pad="24"/>
<connect gate="G$1" pin="P0[2]/A/I/M" pad="25"/>
<connect gate="G$1" pin="P0[3]/A/I/M" pad="31"/>
<connect gate="G$1" pin="P0[4]/A/I/M" pad="26"/>
<connect gate="G$1" pin="P0[5]/A/I/M" pad="30"/>
<connect gate="G$1" pin="P0[6]/A/I/M" pad="27"/>
<connect gate="G$1" pin="P0[7]/A/I/M" pad="29"/>
<connect gate="G$1" pin="P2[0]/M" pad="20"/>
<connect gate="G$1" pin="P2[2]/M" pad="21"/>
<connect gate="G$1" pin="P2[4]/M" pad="22"/>
<connect gate="G$1" pin="P2[6]/M" pad="23"/>
<connect gate="G$1" pin="P3[0]/M" pad="18"/>
<connect gate="G$1" pin="P3[2]/M" pad="19"/>
<connect gate="G$1" pin="SMP" pad="6"/>
<connect gate="G$1" pin="VDD" pad="28"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
<connect gate="G$1" pin="VSS@2" pad="32"/>
<connect gate="G$1" pin="XRES" pad="17"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C58LPXXX" prefix="IC">
<description>&lt;b&gt;CY8C58LPXXX_TQFP100_4JTAG&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: CY8C58LPXXX_TQFP100_4JTAG.bsdl</description>
<gates>
<gate name="G$1" symbol="CY8C58LPXXX_TQFP100_4JTAG"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="IND" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="40"/>
<connect gate="G$1" pin="NC@2" pad="41"/>
<connect gate="G$1" pin="NC@3" pad="57"/>
<connect gate="G$1" pin="NC@4" pad="58"/>
<connect gate="G$1" pin="NC@5" pad="59"/>
<connect gate="G$1" pin="NC@6" pad="60"/>
<connect gate="G$1" pin="NC@7" pad="61"/>
<connect gate="G$1" pin="NC@8" pad="62"/>
<connect gate="G$1" pin="P0_0" pad="71"/>
<connect gate="G$1" pin="P0_1" pad="72"/>
<connect gate="G$1" pin="P0_2" pad="73"/>
<connect gate="G$1" pin="P0_3" pad="74"/>
<connect gate="G$1" pin="P0_4" pad="76"/>
<connect gate="G$1" pin="P0_5" pad="77"/>
<connect gate="G$1" pin="P0_6" pad="78"/>
<connect gate="G$1" pin="P0_7" pad="79"/>
<connect gate="G$1" pin="P12_0" pad="53"/>
<connect gate="G$1" pin="P12_1" pad="54"/>
<connect gate="G$1" pin="P12_2" pad="67"/>
<connect gate="G$1" pin="P12_3" pad="68"/>
<connect gate="G$1" pin="P12_4" pad="4"/>
<connect gate="G$1" pin="P12_5" pad="5"/>
<connect gate="G$1" pin="P12_6" pad="29"/>
<connect gate="G$1" pin="P12_7" pad="30"/>
<connect gate="G$1" pin="P15_0" pad="42"/>
<connect gate="G$1" pin="P15_1" pad="43"/>
<connect gate="G$1" pin="P15_2" pad="55"/>
<connect gate="G$1" pin="P15_3" pad="56"/>
<connect gate="G$1" pin="P15_4" pad="93"/>
<connect gate="G$1" pin="P15_5" pad="94"/>
<connect gate="G$1" pin="P15_6" pad="35"/>
<connect gate="G$1" pin="P15_7" pad="36"/>
<connect gate="G$1" pin="P1_0" pad="20"/>
<connect gate="G$1" pin="P1_1" pad="21"/>
<connect gate="G$1" pin="P1_2" pad="22"/>
<connect gate="G$1" pin="P1_3" pad="23"/>
<connect gate="G$1" pin="P1_4" pad="24"/>
<connect gate="G$1" pin="P1_5" pad="25"/>
<connect gate="G$1" pin="P1_6" pad="27"/>
<connect gate="G$1" pin="P1_7" pad="28"/>
<connect gate="G$1" pin="P2_0" pad="95"/>
<connect gate="G$1" pin="P2_1" pad="96"/>
<connect gate="G$1" pin="P2_2" pad="97"/>
<connect gate="G$1" pin="P2_3" pad="98"/>
<connect gate="G$1" pin="P2_4" pad="99"/>
<connect gate="G$1" pin="P2_5" pad="1"/>
<connect gate="G$1" pin="P2_6" pad="2"/>
<connect gate="G$1" pin="P2_7" pad="3"/>
<connect gate="G$1" pin="P3_0" pad="44"/>
<connect gate="G$1" pin="P3_1" pad="45"/>
<connect gate="G$1" pin="P3_2" pad="46"/>
<connect gate="G$1" pin="P3_3" pad="47"/>
<connect gate="G$1" pin="P3_4" pad="48"/>
<connect gate="G$1" pin="P3_5" pad="49"/>
<connect gate="G$1" pin="P3_6" pad="51"/>
<connect gate="G$1" pin="P3_7" pad="52"/>
<connect gate="G$1" pin="P4_0" pad="69"/>
<connect gate="G$1" pin="P4_1" pad="70"/>
<connect gate="G$1" pin="P4_2" pad="80"/>
<connect gate="G$1" pin="P4_3" pad="81"/>
<connect gate="G$1" pin="P4_4" pad="82"/>
<connect gate="G$1" pin="P4_5" pad="83"/>
<connect gate="G$1" pin="P4_6" pad="84"/>
<connect gate="G$1" pin="P4_7" pad="85"/>
<connect gate="G$1" pin="P5_0" pad="16"/>
<connect gate="G$1" pin="P5_1" pad="17"/>
<connect gate="G$1" pin="P5_2" pad="18"/>
<connect gate="G$1" pin="P5_3" pad="19"/>
<connect gate="G$1" pin="P5_4" pad="31"/>
<connect gate="G$1" pin="P5_5" pad="32"/>
<connect gate="G$1" pin="P5_6" pad="33"/>
<connect gate="G$1" pin="P5_7" pad="34"/>
<connect gate="G$1" pin="P6_0" pad="89"/>
<connect gate="G$1" pin="P6_1" pad="90"/>
<connect gate="G$1" pin="P6_2" pad="91"/>
<connect gate="G$1" pin="P6_3" pad="92"/>
<connect gate="G$1" pin="P6_4" pad="6"/>
<connect gate="G$1" pin="P6_5" pad="7"/>
<connect gate="G$1" pin="P6_6" pad="8"/>
<connect gate="G$1" pin="P6_7" pad="9"/>
<connect gate="G$1" pin="VB" pad="12"/>
<connect gate="G$1" pin="VBAT" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="63"/>
<connect gate="G$1" pin="VCCD@0" pad="39"/>
<connect gate="G$1" pin="VCCD@1" pad="86"/>
<connect gate="G$1" pin="VDDA" pad="65"/>
<connect gate="G$1" pin="VDDD" pad="37"/>
<connect gate="G$1" pin="VDDD@1" pad="88"/>
<connect gate="G$1" pin="VIO0" pad="75"/>
<connect gate="G$1" pin="VIO1" pad="26"/>
<connect gate="G$1" pin="VIO2" pad="100"/>
<connect gate="G$1" pin="VIO3" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="64"/>
<connect gate="G$1" pin="VSSB" pad="10"/>
<connect gate="G$1" pin="VSSD@0" pad="14"/>
<connect gate="G$1" pin="VSSD@0@1" pad="38"/>
<connect gate="G$1" pin="VSSD@1" pad="66"/>
<connect gate="G$1" pin="VSSD@1@1" pad="87"/>
<connect gate="G$1" pin="XRES_N" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C58LPXXX_5JTAG" prefix="IC">
<description>&lt;b&gt;CY8C58LPXXX_TQFP100_5JTAG&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: CY8C58LPXXX_TQFP100_5JTAG.bsdl</description>
<gates>
<gate name="G$1" symbol="CY8C58LPXXX_TQFP100_5JTAG"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="IND" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="40"/>
<connect gate="G$1" pin="NC@2" pad="41"/>
<connect gate="G$1" pin="NC@3" pad="57"/>
<connect gate="G$1" pin="NC@4" pad="58"/>
<connect gate="G$1" pin="NC@5" pad="59"/>
<connect gate="G$1" pin="NC@6" pad="60"/>
<connect gate="G$1" pin="NC@7" pad="61"/>
<connect gate="G$1" pin="NC@8" pad="62"/>
<connect gate="G$1" pin="P0_0" pad="71"/>
<connect gate="G$1" pin="P0_1" pad="72"/>
<connect gate="G$1" pin="P0_2" pad="73"/>
<connect gate="G$1" pin="P0_3" pad="74"/>
<connect gate="G$1" pin="P0_4" pad="76"/>
<connect gate="G$1" pin="P0_5" pad="77"/>
<connect gate="G$1" pin="P0_6" pad="78"/>
<connect gate="G$1" pin="P0_7" pad="79"/>
<connect gate="G$1" pin="P12_0" pad="53"/>
<connect gate="G$1" pin="P12_1" pad="54"/>
<connect gate="G$1" pin="P12_2" pad="67"/>
<connect gate="G$1" pin="P12_3" pad="68"/>
<connect gate="G$1" pin="P12_4" pad="4"/>
<connect gate="G$1" pin="P12_5" pad="5"/>
<connect gate="G$1" pin="P12_6" pad="29"/>
<connect gate="G$1" pin="P12_7" pad="30"/>
<connect gate="G$1" pin="P15_0" pad="42"/>
<connect gate="G$1" pin="P15_1" pad="43"/>
<connect gate="G$1" pin="P15_2" pad="55"/>
<connect gate="G$1" pin="P15_3" pad="56"/>
<connect gate="G$1" pin="P15_4" pad="93"/>
<connect gate="G$1" pin="P15_5" pad="94"/>
<connect gate="G$1" pin="P15_6" pad="35"/>
<connect gate="G$1" pin="P15_7" pad="36"/>
<connect gate="G$1" pin="P1_0" pad="20"/>
<connect gate="G$1" pin="P1_1" pad="21"/>
<connect gate="G$1" pin="P1_2" pad="22"/>
<connect gate="G$1" pin="P1_3" pad="23"/>
<connect gate="G$1" pin="P1_4" pad="24"/>
<connect gate="G$1" pin="P1_5" pad="25"/>
<connect gate="G$1" pin="P1_6" pad="27"/>
<connect gate="G$1" pin="P1_7" pad="28"/>
<connect gate="G$1" pin="P2_0" pad="95"/>
<connect gate="G$1" pin="P2_1" pad="96"/>
<connect gate="G$1" pin="P2_2" pad="97"/>
<connect gate="G$1" pin="P2_3" pad="98"/>
<connect gate="G$1" pin="P2_4" pad="99"/>
<connect gate="G$1" pin="P2_5" pad="1"/>
<connect gate="G$1" pin="P2_6" pad="2"/>
<connect gate="G$1" pin="P2_7" pad="3"/>
<connect gate="G$1" pin="P3_0" pad="44"/>
<connect gate="G$1" pin="P3_1" pad="45"/>
<connect gate="G$1" pin="P3_2" pad="46"/>
<connect gate="G$1" pin="P3_3" pad="47"/>
<connect gate="G$1" pin="P3_4" pad="48"/>
<connect gate="G$1" pin="P3_5" pad="49"/>
<connect gate="G$1" pin="P3_6" pad="51"/>
<connect gate="G$1" pin="P3_7" pad="52"/>
<connect gate="G$1" pin="P4_0" pad="69"/>
<connect gate="G$1" pin="P4_1" pad="70"/>
<connect gate="G$1" pin="P4_2" pad="80"/>
<connect gate="G$1" pin="P4_3" pad="81"/>
<connect gate="G$1" pin="P4_4" pad="82"/>
<connect gate="G$1" pin="P4_5" pad="83"/>
<connect gate="G$1" pin="P4_6" pad="84"/>
<connect gate="G$1" pin="P4_7" pad="85"/>
<connect gate="G$1" pin="P5_0" pad="16"/>
<connect gate="G$1" pin="P5_1" pad="17"/>
<connect gate="G$1" pin="P5_2" pad="18"/>
<connect gate="G$1" pin="P5_3" pad="19"/>
<connect gate="G$1" pin="P5_4" pad="31"/>
<connect gate="G$1" pin="P5_5" pad="32"/>
<connect gate="G$1" pin="P5_6" pad="33"/>
<connect gate="G$1" pin="P5_7" pad="34"/>
<connect gate="G$1" pin="P6_0" pad="89"/>
<connect gate="G$1" pin="P6_1" pad="90"/>
<connect gate="G$1" pin="P6_2" pad="91"/>
<connect gate="G$1" pin="P6_3" pad="92"/>
<connect gate="G$1" pin="P6_4" pad="6"/>
<connect gate="G$1" pin="P6_5" pad="7"/>
<connect gate="G$1" pin="P6_6" pad="8"/>
<connect gate="G$1" pin="P6_7" pad="9"/>
<connect gate="G$1" pin="VB" pad="12"/>
<connect gate="G$1" pin="VBAT" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="63"/>
<connect gate="G$1" pin="VCCD@0" pad="39"/>
<connect gate="G$1" pin="VCCD@1" pad="86"/>
<connect gate="G$1" pin="VDDA" pad="65"/>
<connect gate="G$1" pin="VDDD" pad="37"/>
<connect gate="G$1" pin="VDDD@1" pad="88"/>
<connect gate="G$1" pin="VIO0" pad="75"/>
<connect gate="G$1" pin="VIO1" pad="26"/>
<connect gate="G$1" pin="VIO2" pad="100"/>
<connect gate="G$1" pin="VIO3" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="64"/>
<connect gate="G$1" pin="VSSB" pad="10"/>
<connect gate="G$1" pin="VSSD@0" pad="14"/>
<connect gate="G$1" pin="VSSD@0@1" pad="38"/>
<connect gate="G$1" pin="VSSD@1" pad="66"/>
<connect gate="G$1" pin="VSSD@1@1" pad="87"/>
<connect gate="G$1" pin="XRES_N" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C58LPXXX_USB_4JTAG" prefix="IC">
<description>&lt;b&gt;CY8C58LPXXX_TQFP100_USB_4JTAG&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: CY8C58LPXXX_TQFP100_USB_4JTAG.bsdl</description>
<gates>
<gate name="G$1" symbol="CY8C58LPXXX_TQFP100_USB_4JTAG"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="IND" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="40"/>
<connect gate="G$1" pin="NC@2" pad="41"/>
<connect gate="G$1" pin="NC@3" pad="57"/>
<connect gate="G$1" pin="NC@4" pad="58"/>
<connect gate="G$1" pin="NC@5" pad="59"/>
<connect gate="G$1" pin="NC@6" pad="60"/>
<connect gate="G$1" pin="NC@7" pad="61"/>
<connect gate="G$1" pin="NC@8" pad="62"/>
<connect gate="G$1" pin="P0_0" pad="71"/>
<connect gate="G$1" pin="P0_1" pad="72"/>
<connect gate="G$1" pin="P0_2" pad="73"/>
<connect gate="G$1" pin="P0_3" pad="74"/>
<connect gate="G$1" pin="P0_4" pad="76"/>
<connect gate="G$1" pin="P0_5" pad="77"/>
<connect gate="G$1" pin="P0_6" pad="78"/>
<connect gate="G$1" pin="P0_7" pad="79"/>
<connect gate="G$1" pin="P12_0" pad="53"/>
<connect gate="G$1" pin="P12_1" pad="54"/>
<connect gate="G$1" pin="P12_2" pad="67"/>
<connect gate="G$1" pin="P12_3" pad="68"/>
<connect gate="G$1" pin="P12_4" pad="4"/>
<connect gate="G$1" pin="P12_5" pad="5"/>
<connect gate="G$1" pin="P12_6" pad="29"/>
<connect gate="G$1" pin="P12_7" pad="30"/>
<connect gate="G$1" pin="P15_0" pad="42"/>
<connect gate="G$1" pin="P15_1" pad="43"/>
<connect gate="G$1" pin="P15_2" pad="55"/>
<connect gate="G$1" pin="P15_3" pad="56"/>
<connect gate="G$1" pin="P15_4" pad="93"/>
<connect gate="G$1" pin="P15_5" pad="94"/>
<connect gate="G$1" pin="P1_0" pad="20"/>
<connect gate="G$1" pin="P1_1" pad="21"/>
<connect gate="G$1" pin="P1_2" pad="22"/>
<connect gate="G$1" pin="P1_3" pad="23"/>
<connect gate="G$1" pin="P1_4" pad="24"/>
<connect gate="G$1" pin="P1_5" pad="25"/>
<connect gate="G$1" pin="P1_6" pad="27"/>
<connect gate="G$1" pin="P1_7" pad="28"/>
<connect gate="G$1" pin="P2_0" pad="95"/>
<connect gate="G$1" pin="P2_1" pad="96"/>
<connect gate="G$1" pin="P2_2" pad="97"/>
<connect gate="G$1" pin="P2_3" pad="98"/>
<connect gate="G$1" pin="P2_4" pad="99"/>
<connect gate="G$1" pin="P2_5" pad="1"/>
<connect gate="G$1" pin="P2_6" pad="2"/>
<connect gate="G$1" pin="P2_7" pad="3"/>
<connect gate="G$1" pin="P3_0" pad="44"/>
<connect gate="G$1" pin="P3_1" pad="45"/>
<connect gate="G$1" pin="P3_2" pad="46"/>
<connect gate="G$1" pin="P3_3" pad="47"/>
<connect gate="G$1" pin="P3_4" pad="48"/>
<connect gate="G$1" pin="P3_5" pad="49"/>
<connect gate="G$1" pin="P3_6" pad="51"/>
<connect gate="G$1" pin="P3_7" pad="52"/>
<connect gate="G$1" pin="P4_0" pad="69"/>
<connect gate="G$1" pin="P4_1" pad="70"/>
<connect gate="G$1" pin="P4_2" pad="80"/>
<connect gate="G$1" pin="P4_3" pad="81"/>
<connect gate="G$1" pin="P4_4" pad="82"/>
<connect gate="G$1" pin="P4_5" pad="83"/>
<connect gate="G$1" pin="P4_6" pad="84"/>
<connect gate="G$1" pin="P4_7" pad="85"/>
<connect gate="G$1" pin="P5_0" pad="16"/>
<connect gate="G$1" pin="P5_1" pad="17"/>
<connect gate="G$1" pin="P5_2" pad="18"/>
<connect gate="G$1" pin="P5_3" pad="19"/>
<connect gate="G$1" pin="P5_4" pad="31"/>
<connect gate="G$1" pin="P5_5" pad="32"/>
<connect gate="G$1" pin="P5_6" pad="33"/>
<connect gate="G$1" pin="P5_7" pad="34"/>
<connect gate="G$1" pin="P6_0" pad="89"/>
<connect gate="G$1" pin="P6_1" pad="90"/>
<connect gate="G$1" pin="P6_2" pad="91"/>
<connect gate="G$1" pin="P6_3" pad="92"/>
<connect gate="G$1" pin="P6_4" pad="6"/>
<connect gate="G$1" pin="P6_5" pad="7"/>
<connect gate="G$1" pin="P6_6" pad="8"/>
<connect gate="G$1" pin="P6_7" pad="9"/>
<connect gate="G$1" pin="USB_D+" pad="35"/>
<connect gate="G$1" pin="USB_D-" pad="36"/>
<connect gate="G$1" pin="VB" pad="12"/>
<connect gate="G$1" pin="VBAT" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="63"/>
<connect gate="G$1" pin="VCCD@0" pad="39"/>
<connect gate="G$1" pin="VCCD@1" pad="86"/>
<connect gate="G$1" pin="VDDA" pad="65"/>
<connect gate="G$1" pin="VDDD" pad="37"/>
<connect gate="G$1" pin="VDDD@1" pad="88"/>
<connect gate="G$1" pin="VIO0" pad="75"/>
<connect gate="G$1" pin="VIO1" pad="26"/>
<connect gate="G$1" pin="VIO2" pad="100"/>
<connect gate="G$1" pin="VIO3" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="64"/>
<connect gate="G$1" pin="VSSB" pad="10"/>
<connect gate="G$1" pin="VSSD@0" pad="14"/>
<connect gate="G$1" pin="VSSD@0@1" pad="38"/>
<connect gate="G$1" pin="VSSD@1" pad="66"/>
<connect gate="G$1" pin="VSSD@1@1" pad="87"/>
<connect gate="G$1" pin="XRES_N" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY8C58LPXXX_USB_5JTAG" prefix="IC">
<description>&lt;b&gt;CY8C58LPXXX_TQFP100_USB_5JTAG&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: CY8C58LPXXX_TQFP100_USB_5JTAG.bsdl</description>
<gates>
<gate name="G$1" symbol="CY8C58LPXXX_TQFP100_USB_5JTAG"/>
</gates>
<devices>
<device name="" package="TQFP100-14X14">
<connects>
<connect gate="G$1" pin="IND" pad="11"/>
<connect gate="G$1" pin="NC@1" pad="40"/>
<connect gate="G$1" pin="NC@2" pad="41"/>
<connect gate="G$1" pin="NC@3" pad="57"/>
<connect gate="G$1" pin="NC@4" pad="58"/>
<connect gate="G$1" pin="NC@5" pad="59"/>
<connect gate="G$1" pin="NC@6" pad="60"/>
<connect gate="G$1" pin="NC@7" pad="61"/>
<connect gate="G$1" pin="NC@8" pad="62"/>
<connect gate="G$1" pin="P0_0" pad="71"/>
<connect gate="G$1" pin="P0_1" pad="72"/>
<connect gate="G$1" pin="P0_2" pad="73"/>
<connect gate="G$1" pin="P0_3" pad="74"/>
<connect gate="G$1" pin="P0_4" pad="76"/>
<connect gate="G$1" pin="P0_5" pad="77"/>
<connect gate="G$1" pin="P0_6" pad="78"/>
<connect gate="G$1" pin="P0_7" pad="79"/>
<connect gate="G$1" pin="P12_0" pad="53"/>
<connect gate="G$1" pin="P12_1" pad="54"/>
<connect gate="G$1" pin="P12_2" pad="67"/>
<connect gate="G$1" pin="P12_3" pad="68"/>
<connect gate="G$1" pin="P12_4" pad="4"/>
<connect gate="G$1" pin="P12_5" pad="5"/>
<connect gate="G$1" pin="P12_6" pad="29"/>
<connect gate="G$1" pin="P12_7" pad="30"/>
<connect gate="G$1" pin="P15_0" pad="42"/>
<connect gate="G$1" pin="P15_1" pad="43"/>
<connect gate="G$1" pin="P15_2" pad="55"/>
<connect gate="G$1" pin="P15_3" pad="56"/>
<connect gate="G$1" pin="P15_4" pad="93"/>
<connect gate="G$1" pin="P15_5" pad="94"/>
<connect gate="G$1" pin="P1_0" pad="20"/>
<connect gate="G$1" pin="P1_1" pad="21"/>
<connect gate="G$1" pin="P1_2" pad="22"/>
<connect gate="G$1" pin="P1_3" pad="23"/>
<connect gate="G$1" pin="P1_4" pad="24"/>
<connect gate="G$1" pin="P1_5" pad="25"/>
<connect gate="G$1" pin="P1_6" pad="27"/>
<connect gate="G$1" pin="P1_7" pad="28"/>
<connect gate="G$1" pin="P2_0" pad="95"/>
<connect gate="G$1" pin="P2_1" pad="96"/>
<connect gate="G$1" pin="P2_2" pad="97"/>
<connect gate="G$1" pin="P2_3" pad="98"/>
<connect gate="G$1" pin="P2_4" pad="99"/>
<connect gate="G$1" pin="P2_5" pad="1"/>
<connect gate="G$1" pin="P2_6" pad="2"/>
<connect gate="G$1" pin="P2_7" pad="3"/>
<connect gate="G$1" pin="P3_0" pad="44"/>
<connect gate="G$1" pin="P3_1" pad="45"/>
<connect gate="G$1" pin="P3_2" pad="46"/>
<connect gate="G$1" pin="P3_3" pad="47"/>
<connect gate="G$1" pin="P3_4" pad="48"/>
<connect gate="G$1" pin="P3_5" pad="49"/>
<connect gate="G$1" pin="P3_6" pad="51"/>
<connect gate="G$1" pin="P3_7" pad="52"/>
<connect gate="G$1" pin="P4_0" pad="69"/>
<connect gate="G$1" pin="P4_1" pad="70"/>
<connect gate="G$1" pin="P4_2" pad="80"/>
<connect gate="G$1" pin="P4_3" pad="81"/>
<connect gate="G$1" pin="P4_4" pad="82"/>
<connect gate="G$1" pin="P4_5" pad="83"/>
<connect gate="G$1" pin="P4_6" pad="84"/>
<connect gate="G$1" pin="P4_7" pad="85"/>
<connect gate="G$1" pin="P5_0" pad="16"/>
<connect gate="G$1" pin="P5_1" pad="17"/>
<connect gate="G$1" pin="P5_2" pad="18"/>
<connect gate="G$1" pin="P5_3" pad="19"/>
<connect gate="G$1" pin="P5_4" pad="31"/>
<connect gate="G$1" pin="P5_5" pad="32"/>
<connect gate="G$1" pin="P5_6" pad="33"/>
<connect gate="G$1" pin="P5_7" pad="34"/>
<connect gate="G$1" pin="P6_0" pad="89"/>
<connect gate="G$1" pin="P6_1" pad="90"/>
<connect gate="G$1" pin="P6_2" pad="91"/>
<connect gate="G$1" pin="P6_3" pad="92"/>
<connect gate="G$1" pin="P6_4" pad="6"/>
<connect gate="G$1" pin="P6_5" pad="7"/>
<connect gate="G$1" pin="P6_6" pad="8"/>
<connect gate="G$1" pin="P6_7" pad="9"/>
<connect gate="G$1" pin="USB_D+" pad="35"/>
<connect gate="G$1" pin="USB_D-" pad="36"/>
<connect gate="G$1" pin="VB" pad="12"/>
<connect gate="G$1" pin="VBAT" pad="13"/>
<connect gate="G$1" pin="VCCA" pad="63"/>
<connect gate="G$1" pin="VCCD@0" pad="39"/>
<connect gate="G$1" pin="VCCD@1" pad="86"/>
<connect gate="G$1" pin="VDDA" pad="65"/>
<connect gate="G$1" pin="VDDD" pad="37"/>
<connect gate="G$1" pin="VDDD@1" pad="88"/>
<connect gate="G$1" pin="VIO0" pad="75"/>
<connect gate="G$1" pin="VIO1" pad="26"/>
<connect gate="G$1" pin="VIO2" pad="100"/>
<connect gate="G$1" pin="VIO3" pad="50"/>
<connect gate="G$1" pin="VSSA" pad="64"/>
<connect gate="G$1" pin="VSSB" pad="10"/>
<connect gate="G$1" pin="VSSD@0" pad="14"/>
<connect gate="G$1" pin="VSSD@0@1" pad="38"/>
<connect gate="G$1" pin="VSSD@1" pad="66"/>
<connect gate="G$1" pin="VSSD@1@1" pad="87"/>
<connect gate="G$1" pin="XRES_N" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
