<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.2">
<drawing>
<library>
<description>&lt;b&gt;Kontron / JUMPtec ETX Board&lt;/b&gt;&lt;p&gt;
Source: www.kontron.com/techlib/whitepapers/etx_spec.pdf
JUMPtec&lt;br&gt;
Industrielle Computertechnik AG&lt;br&gt;
Brunnwiesenstr. 16 D-94469 Deggendorf</description>
<packages>
<package name="FX8-100S-SV">
<description>&lt;b&gt;HIROSE - ETX Board Connector&lt;/b&gt; 100 Pos.&lt;p&gt;
Source: 
&lt;ul&gt;
&lt;li&gt;
www.hirose.co.jp/cataloge_hp/e57800016.pdf&lt;br&gt;
&lt;/li&gt;
&lt;li&gt;
www.kontron.com/techlib/whitepapers/etx_spec.pdf&lt;br&gt;
&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
<package name="ETX-BOARD-WITH-CONTACT">
<description>&lt;b&gt;ETX-board&lt;/b&gt; MECHANICAL SPECIFICATION OF BACKPLANE&lt;p&gt;
Board with X1 - X4 Connector&lt;br&gt;
Source: www.kontron.com/techlib/whitepapers/etx_spec.pdf&lt;br&gt;</description>
</package>
<package name="ETX-BOARD-HOLE-POS">
<description>&lt;b&gt;ETX-board&lt;/b&gt; MECHANICAL SPECIFICATION OF BACKPLANE&lt;p&gt;
Board with hole position (without connector)&lt;br&gt;
Source: www.kontron.com/techlib/whitepapers/etx_spec.pdf&lt;br&gt;</description>
</package>
<package name="C-5353652-36-3">
<description>&lt;b&gt;ComExpress&lt;/b&gt; (ETXexpress)&lt;p&gt;
Source: http://catalog.tycoelectronics.com .. ENG_CS_889092_0.5mm_FH_Conn_0906.pdf</description>
</package>
</packages>
<symbols>
<symbol name="X1">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="PCICLK3"/>
<pin name="PCICLK4"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="PCICLK1"/>
<pin name="PCICLK2"/>
<pin name="!REQ3"/>
<pin name="!GNT3"/>
<pin name="!GNT2"/>
<pin name="3V" direction="pwr"/>
<pin name="!REQ2"/>
<pin name="!GNT1"/>
<pin name="!REQ1"/>
<pin name="3V@1" direction="pwr"/>
<pin name="!GNT0"/>
<pin name="RESERVED"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="SERIRQ"/>
<pin name="!REQ0"/>
<pin name="AD0"/>
<pin name="3V@2" direction="pwr"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD4"/>
<pin name="AD3"/>
<pin name="AD6"/>
<pin name="AD5"/>
<pin name="!CBE0"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5"/>
<pin name="AD10"/>
<pin name="AUXAL"/>
<pin name="AD11"/>
<pin name="MIC"/>
<pin name="AD12"/>
<pin name="AUXAR"/>
<pin name="AD13"/>
<pin name="ASVCC" direction="pwr"/>
<pin name="AD14"/>
<pin name="SNDL"/>
<pin name="AD15"/>
<pin name="ASGND" direction="pwr"/>
<pin name="!CBE1"/>
<pin name="SNDR"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="PAR"/>
<pin name="!SERR"/>
<pin name="!GPERR"/>
<pin name="RESERVED@1"/>
<pin name="!PME"/>
<pin name="!USB2"/>
<pin name="!LOCK"/>
<pin name="!DEVSEL"/>
<pin name="!TRDY"/>
<pin name="!USB3"/>
<pin name="!IRDY"/>
<pin name="!STOP"/>
<pin name="!FRAME"/>
<pin name="USB2"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="AD16"/>
<pin name="!CBE2"/>
<pin name="AD17"/>
<pin name="USB3"/>
<pin name="AD19"/>
<pin name="AD18"/>
<pin name="AD20"/>
<pin name="!USB0"/>
<pin name="AD22"/>
<pin name="AD21"/>
<pin name="AD23"/>
<pin name="!USB1"/>
<pin name="AD24"/>
<pin name="!CBE3"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD28"/>
<pin name="USB0"/>
<pin name="AD27"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="USB1"/>
<pin name="!PCIRST"/>
<pin name="AD31"/>
<pin name="!INTC"/>
<pin name="!INTD"/>
<pin name="!INTA"/>
<pin name="!INTB"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
</symbol>
<symbol name="X2">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="SD14"/>
<pin name="SD15"/>
<pin name="SD13"/>
<pin name="!MASTER"/>
<pin name="SD12"/>
<pin name="DREQ7"/>
<pin name="SD11"/>
<pin name="!DACK7"/>
<pin name="SD10"/>
<pin name="DREQ6"/>
<pin name="SD9"/>
<pin name="!DACK6"/>
<pin name="SD8"/>
<pin name="DREQ5"/>
<pin name="!MEMW"/>
<pin name="!DACK5"/>
<pin name="!MEMR"/>
<pin name="DREQ0"/>
<pin name="LA17"/>
<pin name="!DACK0"/>
<pin name="LA18"/>
<pin name="IRQ14"/>
<pin name="LA19"/>
<pin name="IRQ15"/>
<pin name="LA20"/>
<pin name="IRQ12"/>
<pin name="LA21"/>
<pin name="IRQ11"/>
<pin name="LA22"/>
<pin name="IRQ10"/>
<pin name="LA23"/>
<pin name="!IO16"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="!SBHE"/>
<pin name="!M16"/>
<pin name="SA0"/>
<pin name="OSC"/>
<pin name="SA1"/>
<pin name="BALE"/>
<pin name="SA2"/>
<pin name="TC"/>
<pin name="SA3"/>
<pin name="!DACK2"/>
<pin name="SA4"/>
<pin name="IRQ3"/>
<pin name="SA5"/>
<pin name="IRQ4"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="SA6"/>
<pin name="IRQ5"/>
<pin name="SA7"/>
<pin name="IRQ6"/>
<pin name="SA8"/>
<pin name="IRQ7"/>
<pin name="SA9"/>
<pin name="SYSCLK"/>
<pin name="SA10"/>
<pin name="!REFSH"/>
<pin name="SA11"/>
<pin name="DREQ1"/>
<pin name="SA12"/>
<pin name="!DACK1"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="SA13"/>
<pin name="DREQ3"/>
<pin name="SA14"/>
<pin name="!DACK3"/>
<pin name="SA15"/>
<pin name="!IOR"/>
<pin name="SA16"/>
<pin name="!IOW"/>
<pin name="SA18"/>
<pin name="SA17"/>
<pin name="SA19"/>
<pin name="!SMEMR"/>
<pin name="IOCHRDY"/>
<pin name="AEN"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="SD0"/>
<pin name="!SMEMW"/>
<pin name="SD2"/>
<pin name="SD1"/>
<pin name="SD3"/>
<pin name="!NOWS"/>
<pin name="DREQ2"/>
<pin name="SD4"/>
<pin name="SD5"/>
<pin name="IRQ9"/>
<pin name="SD6"/>
<pin name="SD7"/>
<pin name="!IOCHK"/>
<pin name="RSTDRV"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
</symbol>
<symbol name="X3-ANALOG">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="R"/>
<pin name="B"/>
<pin name="HSY"/>
<pin name="G"/>
<pin name="VSY"/>
<pin name="DDCK"/>
<pin name="!DETECT"/>
<pin name="DDDA"/>
<pin name="B4"/>
<pin name="LCDDO18"/>
<pin name="B5"/>
<pin name="EN"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="B1"/>
<pin name="B3"/>
<pin name="B0"/>
<pin name="B2"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="G2"/>
<pin name="G5"/>
<pin name="G3"/>
<pin name="G4"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="LCDDO4"/>
<pin name="G1"/>
<pin name="LCDDO5"/>
<pin name="G0"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="LCDDO1"/>
<pin name="LCDDO3"/>
<pin name="LCDDO0"/>
<pin name="LCDDO2"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="JILI_DAT"/>
<pin name="LTGIO0"/>
<pin name="JILI_CLK"/>
<pin name="!BLON"/>
<pin name="BIASON"/>
<pin name="DIGON"/>
<pin name="COMP"/>
<pin name="Y"/>
<pin name="SYNC"/>
<pin name="C"/>
<pin name="LPT/!FLPY"/>
<pin name="RESERVED"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="RESERVED@1"/>
<pin name="!AFD"/>
<pin name="RESERVED@2"/>
<pin name="PD7"/>
<pin name="IRRX"/>
<pin name="!ERR"/>
<pin name="IRTX"/>
<pin name="PD6"/>
<pin name="RXD2"/>
<pin name="!DIR"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="!RTS2"/>
<pin name="PD5"/>
<pin name="!DTR2"/>
<pin name="!SLIN"/>
<pin name="!DCD2"/>
<pin name="!DSKCHG"/>
<pin name="!DSR2"/>
<pin name="PD3"/>
<pin name="!CTS2"/>
<pin name="PD2"/>
<pin name="TXD2"/>
<pin name="PD1"/>
<pin name="!RI2"/>
<pin name="!INDEX"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="RXD1"/>
<pin name="!ACK"/>
<pin name="!RTS1"/>
<pin name="BUSY"/>
<pin name="!DTR1"/>
<pin name="PE"/>
<pin name="!DCD1"/>
<pin name="!SLCT"/>
<pin name="!DSR1"/>
<pin name="MSCLK"/>
<pin name="!CTS1"/>
<pin name="MSDAT"/>
<pin name="TXD1"/>
<pin name="KBCLK"/>
<pin name="!RI1"/>
<pin name="KBDAT"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
</symbol>
<symbol name="X3-LVDS">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="R"/>
<pin name="B"/>
<pin name="HSY"/>
<pin name="G"/>
<pin name="VSY"/>
<pin name="DDCK"/>
<pin name="!DETECT"/>
<pin name="DDDA"/>
<pin name="LCDDO16"/>
<pin name="SHFCLK"/>
<pin name="LCDDO17"/>
<pin name="LCDDO19"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="LCDDO13"/>
<pin name="LCDDO15"/>
<pin name="LCDDO12"/>
<pin name="LCDDO14"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="LCDDO8"/>
<pin name="LCDDO11"/>
<pin name="LCDDO9"/>
<pin name="LCDDO10"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="R4"/>
<pin name="LCDDO7"/>
<pin name="R5"/>
<pin name="LCDDO6"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="R1"/>
<pin name="R3"/>
<pin name="R0"/>
<pin name="R2"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="JILI_DAT"/>
<pin name="VSYNC"/>
<pin name="JILI_CLK"/>
<pin name="!BLON"/>
<pin name="HSYNC"/>
<pin name="DIGON"/>
<pin name="COMP"/>
<pin name="Y"/>
<pin name="SYNC"/>
<pin name="C"/>
<pin name="LPT/!FLPY"/>
<pin name="RESERVED"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="!STB"/>
<pin name="DENSEL"/>
<pin name="RESERVED@1"/>
<pin name="RESERVED@2"/>
<pin name="IRRX"/>
<pin name="!HDSEL"/>
<pin name="IRTX"/>
<pin name="RESERVED@3"/>
<pin name="RXD2"/>
<pin name="!INIT"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="!RTS2"/>
<pin name="RESERVED@4"/>
<pin name="!DTR2"/>
<pin name="!STEP"/>
<pin name="!DCD2"/>
<pin name="PD4"/>
<pin name="!DSR2"/>
<pin name="!RDATA"/>
<pin name="!CTS2"/>
<pin name="!WP"/>
<pin name="TXD2"/>
<pin name="!TRK0"/>
<pin name="!RI2"/>
<pin name="PD0"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="RXD1"/>
<pin name="DRV"/>
<pin name="!RTS1"/>
<pin name="MOT"/>
<pin name="!DTR1"/>
<pin name="!WDATA"/>
<pin name="!DCD1"/>
<pin name="!WGATE"/>
<pin name="!DSR1"/>
<pin name="MSCLK"/>
<pin name="!CTS1"/>
<pin name="MSDAT"/>
<pin name="TXD1"/>
<pin name="KBCLK"/>
<pin name="!RI1"/>
<pin name="KBDAT"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
</symbol>
<symbol name="X4">
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="5V_SB"/>
<pin name="PWGIN"/>
<pin name="PS_ON"/>
<pin name="SPEAKER"/>
<pin name="!PWRBTN"/>
<pin name="BATT"/>
<pin name="!KBINH"/>
<pin name="!LILED"/>
<pin name="!RSMRST"/>
<pin name="!ACTLED"/>
<pin name="!ROMKBCS"/>
<pin name="!SPEEDLED"/>
<pin name="EXT_PRG"/>
<pin name="I2CLK"/>
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="!OVCR"/>
<pin name="!GPCS"/>
<pin name="!EXTSMI"/>
<pin name="I2DAT"/>
<pin name="SMBCLK"/>
<pin name="SMBDATA"/>
<pin name="!SIDE_CS3"/>
<pin name="!SMBALRT"/>
<pin name="!SIDE_CS1"/>
<pin name="DASP_S"/>
<pin name="SIDE_A2"/>
<pin name="!PIDE_CS3"/>
<pin name="SIDE_A0"/>
<pin name="!PIDE_CS1"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="PDIAG_S"/>
<pin name="PIDE_A2"/>
<pin name="SIDE_A1"/>
<pin name="PIDE_A0"/>
<pin name="SIDE_INTRQ"/>
<pin name="PIDE_A1"/>
<pin name="!BATLOW"/>
<pin name="!GPE1"/>
<pin name="!SIDE_AK"/>
<pin name="PIDE_INTRQ"/>
<pin name="SIDE_RDY"/>
<pin name="!PIDE_AK"/>
<pin name="!SIDE_IOR"/>
<pin name="PIDE_RDY"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="!SIDE_IOW"/>
<pin name="!PIDE_IOR"/>
<pin name="SIDE_DRQ"/>
<pin name="!PIDE_IOW"/>
<pin name="SIDE_D15"/>
<pin name="PIDE_DRQ"/>
<pin name="SIDE_D0"/>
<pin name="PIDE_D15"/>
<pin name="SIDE_D14"/>
<pin name="PIDE_D0"/>
<pin name="SIDE_D1"/>
<pin name="PIDE_D14"/>
<pin name="SIDE_D13"/>
<pin name="PIDE_D1"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="SIDE_D2"/>
<pin name="PIDE_D13"/>
<pin name="SIDE_D12"/>
<pin name="PIDE_D2"/>
<pin name="SIDE_D3"/>
<pin name="PIDE_D12"/>
<pin name="SIDE_D11"/>
<pin name="PIDE_D3"/>
<pin name="SIDE_D4"/>
<pin name="PIDE_D11"/>
<pin name="SIDE_D10"/>
<pin name="PIDE_D4"/>
<pin name="SIDE_D5"/>
<pin name="PIDE_D10"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="SIDE_D9"/>
<pin name="PIDE_D5"/>
<pin name="SIDE_D6"/>
<pin name="PIDE_D9"/>
<pin name="SIDE_D8"/>
<pin name="PIDE_D6"/>
<pin name="!GPE2"/>
<pin name="CBLID_P"/>
<pin name="!RXD"/>
<pin name="PIDE_D8"/>
<pin name="RXD"/>
<pin name="SIDE_D7"/>
<pin name="!TXD"/>
<pin name="PIDE_D7"/>
<pin name="TXD"/>
<pin name="!HDRST"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
</symbol>
<symbol name="COMEXPRESS">
<pin name="GND" direction="pas"/>
<pin name="GBE0_MDI3-" direction="pas"/>
<pin name="GBE0_MDI3+" direction="pas"/>
<pin name="GBE0_LINK10" direction="pas"/>
<pin name="GBE0_LINK10@1" direction="pas"/>
<pin name="GBE0_MDI2-" direction="pas"/>
<pin name="GBE0_MDI2+" direction="pas"/>
<pin name="GBE0_!LINK" direction="pas"/>
<pin name="GBE0_MDI1-" direction="pas"/>
<pin name="GBE0_MDI1+" direction="pas"/>
<pin name="GND@1" direction="pas"/>
<pin name="GBE0_MDI0-" direction="pas"/>
<pin name="GBE0_MDI0+" direction="pas"/>
<pin name="GBE0_CTREF" direction="pas"/>
<pin name="!SUS_S3" direction="pas"/>
<pin name="SATA0_TX+" direction="pas"/>
<pin name="SATA0_TX-" direction="pas"/>
<pin name="!SUS_S4" direction="pas"/>
<pin name="SATA0_RX+" direction="pas"/>
<pin name="SATA0_RX-" direction="pas"/>
<pin name="GND@2" direction="pas"/>
<pin name="SATA2_TX+" direction="pas"/>
<pin name="SATA2_TX-" direction="pas"/>
<pin name="!SUS_S5" direction="pas"/>
<pin name="SATA2_RX+" direction="pas"/>
<pin name="SATA2_RX-" direction="pas"/>
<pin name="!BATLOW" direction="pas"/>
<pin name="!ATA_ACT" direction="pas"/>
<pin name="AC_SYNC" direction="pas"/>
<pin name="!AC_RST" direction="pas"/>
<pin name="GND@3" direction="pas"/>
<pin name="AC_BITCLK" direction="pas"/>
<pin name="AC_SDOUT" direction="pas"/>
<pin name="BIOS_DISABLE" direction="pas"/>
<pin name="!THRMTRIP" direction="pas"/>
<pin name="USB6-" direction="pas"/>
<pin name="USB6+" direction="pas"/>
<pin name="!USB_6_7_OC" direction="pas"/>
<pin name="USB4-" direction="pas"/>
<pin name="USB4+" direction="pas"/>
<pin name="GND@4" direction="pas"/>
<pin name="USB2-" direction="pas"/>
<pin name="USB2+" direction="pas"/>
<pin name="!USB_2_3_OC" direction="pas"/>
<pin name="USB0-" direction="pas"/>
<pin name="USB0+" direction="pas"/>
<pin name="VCC_RTC" direction="pas"/>
<pin name="!EXCD0_PERST" direction="pas"/>
<pin name="!EXCD0_CPPE" direction="pas"/>
<pin name="LPC_SERIRQ" direction="pas"/>
<pin name="GND@5" direction="pas"/>
<pin name="PCIE_TX5+" direction="pas"/>
<pin name="PCIE_TX5-" direction="pas"/>
<pin name="GPI0" direction="pas"/>
<pin name="PCIE_TX4+" direction="pas"/>
<pin name="PCIE_TX4-" direction="pas"/>
<pin name="GND@6" direction="pas"/>
<pin name="PCIE_TX3+" direction="pas"/>
<pin name="PCIE_TX3-" direction="pas"/>
<pin name="GND@7" direction="pas"/>
<pin name="PCIE_TX2+" direction="pas"/>
<pin name="PCIE_TX2-" direction="pas"/>
<pin name="GPI1" direction="pas"/>
<pin name="PCIE_TX1+" direction="pas"/>
<pin name="PCIE_TX1-" direction="pas"/>
<pin name="GND@8" direction="pas"/>
<pin name="GPI2" direction="pas"/>
<pin name="PCIE_TX0+" direction="pas"/>
<pin name="PCIE_TX0-" direction="pas"/>
<pin name="GND@9" direction="pas"/>
<pin name="LVDS_A0+" direction="pas"/>
<pin name="LVDS_A0-" direction="pas"/>
<pin name="LVDS_A1+" direction="pas"/>
<pin name="LVDS_A1-" direction="pas"/>
<pin name="LVDS_A2+" direction="pas"/>
<pin name="LVDS_A2-" direction="pas"/>
<pin name="LVDS_VDD_EN" direction="pas"/>
<pin name="LVDS_A3+" direction="pas"/>
<pin name="LVDS_A3-" direction="pas"/>
<pin name="GND@10" direction="pas"/>
<pin name="LVDS_A_CK+" direction="pas"/>
<pin name="LVDS_A_CK-" direction="pas"/>
<pin name="LVDS_I2C_CK" direction="pas"/>
<pin name="LVDS_I2C_DAT" direction="pas"/>
<pin name="GPI3" direction="pas"/>
<pin name="!KBD_RST" direction="pas"/>
<pin name="KBD_A20GATE" direction="pas"/>
<pin name="PCIE0_CK_REF+" direction="pas"/>
<pin name="PCIE0_CK_REF-" direction="pas"/>
<pin name="GND@11" direction="pas"/>
<pin name="RSVD" direction="pas"/>
<pin name="RSVD@1" direction="pas"/>
<pin name="GPO0" direction="pas"/>
<pin name="RSVD@2" direction="pas"/>
<pin name="RSVD@3" direction="pas"/>
<pin name="GND@12" direction="pas"/>
<pin name="VCC_12V" direction="pas"/>
<pin name="VCC_12V@1" direction="pas"/>
<pin name="VCC_12V@2" direction="pas"/>
<pin name="GND@13" direction="pas"/>
<pin name="VCC_12V@3" direction="pas"/>
<pin name="VCC_12V@4" direction="pas"/>
<pin name="VCC_12V@5" direction="pas"/>
<pin name="VCC_12V@6" direction="pas"/>
<pin name="VCC_12V@7" direction="pas"/>
<pin name="VCC_12V@8" direction="pas"/>
<pin name="VCC_12V@9" direction="pas"/>
<pin name="VCC_12V@10" direction="pas"/>
<pin name="VCC_12V@11" direction="pas"/>
<pin name="GND@14" direction="pas"/>
<pin name="GND@15" direction="pas"/>
<pin name="GBE0_ACT" direction="pas"/>
<pin name="LPC_FRAME!" direction="pas"/>
<pin name="LPC_AD0" direction="pas"/>
<pin name="LPC_AD1" direction="pas"/>
<pin name="LPC_AD2" direction="pas"/>
<pin name="LPC_AD3" direction="pas"/>
<pin name="!LPC_DRQ0" direction="pas"/>
<pin name="LPC_DRQ1!" direction="pas"/>
<pin name="LPC_CLK" direction="pas"/>
<pin name="GND@16" direction="pas"/>
<pin name="!PWRBTN" direction="pas"/>
<pin name="SMB_CK" direction="pas"/>
<pin name="SMB_DAT" direction="pas"/>
<pin name="SMB_ALERT!" direction="pas"/>
<pin name="SATA1_TX+" direction="pas"/>
<pin name="SATA1_TX-" direction="pas"/>
<pin name="SUS_STAT!" direction="pas"/>
<pin name="SATA1_RX+" direction="pas"/>
<pin name="SATA1_RX-" direction="pas"/>
<pin name="GND@17" direction="pas"/>
<pin name="SATA3_TX+" direction="pas"/>
<pin name="SATA3_TX-" direction="pas"/>
<pin name="PWR_OK" direction="pas"/>
<pin name="SATA3_RX+" direction="pas"/>
<pin name="SATA3_RX-" direction="pas"/>
<pin name="WDT" direction="pas"/>
<pin name="AC_SDIN2" direction="pas"/>
<pin name="AC_SDIN1" direction="pas"/>
<pin name="AC_SDIN0" direction="pas"/>
<pin name="GND@18" direction="pas"/>
<pin name="SPKR" direction="pas"/>
<pin name="I2C_CK" direction="pas"/>
<pin name="I2C_DAT" direction="pas"/>
<pin name="THRM!" direction="pas"/>
<pin name="USB7-" direction="pas"/>
<pin name="USB7+" direction="pas"/>
<pin name="!USB_4_5_OC" direction="pas"/>
<pin name="USB5-" direction="pas"/>
<pin name="USB5+" direction="pas"/>
<pin name="GND@19" direction="pas"/>
<pin name="USB3-" direction="pas"/>
<pin name="USB3+" direction="pas"/>
<pin name="!USB_0_1_OC" direction="pas"/>
<pin name="USB1-" direction="pas"/>
<pin name="USB1+" direction="pas"/>
<pin name="!EXCD1_PERST" direction="pas"/>
<pin name="!EXCD1_CPPE" direction="pas"/>
<pin name="!SYS_RESET" direction="pas"/>
<pin name="!CB_RESET" direction="pas"/>
<pin name="GND@20" direction="pas"/>
<pin name="PCIE_RX5+" direction="pas"/>
<pin name="PCIE_RX5-" direction="pas"/>
<pin name="GPO1" direction="pas"/>
<pin name="PCIE_RX4+" direction="pas"/>
<pin name="PCIE_RX4-" direction="pas"/>
<pin name="GPO2" direction="pas"/>
<pin name="PCIE_RX3+" direction="pas"/>
<pin name="PCIE_RX3-" direction="pas"/>
<pin name="GND@21" direction="pas"/>
<pin name="PCIE_RX2+" direction="pas"/>
<pin name="PCIE_RX2-" direction="pas"/>
<pin name="GPO3" direction="pas"/>
<pin name="PCIE_RX1+" direction="pas"/>
<pin name="PCIE_RX1-" direction="pas"/>
<pin name="!WAKE0" direction="pas"/>
<pin name="!WAKE1" direction="pas"/>
<pin name="PCIE_RX0+" direction="pas"/>
<pin name="PCIE_RX0-" direction="pas"/>
<pin name="GND@22" direction="pas"/>
<pin name="LVDS_B0+" direction="pas"/>
<pin name="LVDS_B0-" direction="pas"/>
<pin name="LVDS_B1+" direction="pas"/>
<pin name="LVDS_B1-" direction="pas"/>
<pin name="LVDS_B2+" direction="pas"/>
<pin name="LVDS_B2-" direction="pas"/>
<pin name="LVDS_B3+" direction="pas"/>
<pin name="LVDS_B3-" direction="pas"/>
<pin name="LVDS_BKLT_EN" direction="pas"/>
<pin name="GND@23" direction="pas"/>
<pin name="LVDS_B_CK+" direction="pas"/>
<pin name="LVDS_B_CK-" direction="pas"/>
<pin name="LVDS_BKLT_CTRL" direction="pas"/>
<pin name="VCC_5V_SBY" direction="pas"/>
<pin name="VCC_5V_SBY@1" direction="pas"/>
<pin name="VCC_5V_SBY@2" direction="pas"/>
<pin name="VCC_5V_SBY@3" direction="pas"/>
<pin name="RSVD@4" direction="pas"/>
<pin name="VGA_RED" direction="pas"/>
<pin name="GND@24" direction="pas"/>
<pin name="VGA_GRN" direction="pas"/>
<pin name="VGA_BLU" direction="pas"/>
<pin name="VGA_HSYNC" direction="pas"/>
<pin name="VGA_VSYNC" direction="pas"/>
<pin name="VGA_I2C_CK" direction="pas"/>
<pin name="VGA_I2C_DAT" direction="pas"/>
<pin name="TV_DAC_A" direction="pas"/>
<pin name="TV_DAC_B" direction="pas"/>
<pin name="TV_DAC_C" direction="pas"/>
<pin name="GND@25" direction="pas"/>
<pin name="VCC_12V@12" direction="pas"/>
<pin name="VCC_12V@13" direction="pas"/>
<pin name="VCC_12V@14" direction="pas"/>
<pin name="VCC_12V@15" direction="pas"/>
<pin name="VCC_12V@16" direction="pas"/>
<pin name="VCC_12V@17" direction="pas"/>
<pin name="VCC_12V@18" direction="pas"/>
<pin name="VCC_12V@19" direction="pas"/>
<pin name="VCC_12V@20" direction="pas"/>
<pin name="GND@26" direction="pas"/>
<pin name="GND@27" direction="pas"/>
<pin name="IDE_D7" direction="pas"/>
<pin name="IDE_D6" direction="pas"/>
<pin name="IDE_D3" direction="pas"/>
<pin name="IDE_D15" direction="pas"/>
<pin name="IDE_D8" direction="pas"/>
<pin name="IDE_D9" direction="pas"/>
<pin name="IDE_D2" direction="pas"/>
<pin name="IDE_D13" direction="pas"/>
<pin name="IDE_D1" direction="pas"/>
<pin name="GND@28" direction="pas"/>
<pin name="IDE_D14" direction="pas"/>
<pin name="IDE_IORDY" direction="pas"/>
<pin name="!IDE_IOR" direction="pas"/>
<pin name="!PCI_PME" direction="pas"/>
<pin name="!PCI_GNT2" direction="pas"/>
<pin name="!PCI_REQ2" direction="pas"/>
<pin name="!PCI_GNT1" direction="pas"/>
<pin name="!PCI_REQ1" direction="pas"/>
<pin name="!PCI_GNT0" direction="pas"/>
<pin name="GND@29" direction="pas"/>
<pin name="!PCI_REQ0" direction="pas"/>
<pin name="!PCI_RST" direction="pas"/>
<pin name="PCI_AD0" direction="pas"/>
<pin name="PCI_AD2" direction="pas"/>
<pin name="PCI_AD4" direction="pas"/>
<pin name="PCI_AD6" direction="pas"/>
<pin name="PCI_AD8" direction="pas"/>
<pin name="PCI_AD10" direction="pas"/>
<pin name="PCI_AD12" direction="pas"/>
<pin name="GND@30" direction="pas"/>
<pin name="PCI_AD14" direction="pas"/>
<pin name="PCI_C/!BE1" direction="pas"/>
<pin name="!PCI_PERR" direction="pas"/>
<pin name="!PCI_LOCK" direction="pas"/>
<pin name="!PCI_DEVSEL" direction="pas"/>
<pin name="!PCI_IRDY" direction="pas"/>
<pin name="PCI_C/!BE2" direction="pas"/>
<pin name="PCI_AD17" direction="pas"/>
<pin name="PCI_AD19" direction="pas"/>
<pin name="GND@31" direction="pas"/>
<pin name="PCI_AD21" direction="pas"/>
<pin name="PCI_AD23" direction="pas"/>
<pin name="PCI_C/!BE3" direction="pas"/>
<pin name="PCI_AD25" direction="pas"/>
<pin name="PCI_AD27" direction="pas"/>
<pin name="PCI_AD29" direction="pas"/>
<pin name="PCI_AD31" direction="pas"/>
<pin name="!PCI_IRQA" direction="pas"/>
<pin name="!PCI_IRQB" direction="pas"/>
<pin name="GND@32" direction="pas"/>
<pin name="PEG_RX0+" direction="pas"/>
<pin name="PEG_RX0-" direction="pas"/>
<pin name="!TYPE0" direction="pas"/>
<pin name="PEG_RX1+" direction="pas"/>
<pin name="PEG_RX1-" direction="pas"/>
<pin name="!TYPE1" direction="pas"/>
<pin name="PEG_RX2+" direction="pas"/>
<pin name="PEG_RX2-" direction="pas"/>
<pin name="GND@33" direction="pas"/>
<pin name="PEG_RX3+" direction="pas"/>
<pin name="PEG_RX3-" direction="pas"/>
<pin name="RSVD@5" direction="pas"/>
<pin name="RSVD@6" direction="pas"/>
<pin name="PEG_RX4+" direction="pas"/>
<pin name="PEG_RX4-" direction="pas"/>
<pin name="RSVD@7" direction="pas"/>
<pin name="PEG_RX5+" direction="pas"/>
<pin name="PEG_RX5-" direction="pas"/>
<pin name="GND@34" direction="pas"/>
<pin name="PEG_RX6+" direction="pas"/>
<pin name="PEG_RX6-" direction="pas"/>
<pin name="SDVO_DATA" direction="pas"/>
<pin name="PEG_RX7+" direction="pas"/>
<pin name="PEG_RX7-" direction="pas"/>
<pin name="GND@35" direction="pas"/>
<pin name="RSVD@8" direction="pas"/>
<pin name="PEG_RX8+" direction="pas"/>
<pin name="PEG_RX8-" direction="pas"/>
<pin name="GND@36" direction="pas"/>
<pin name="PEG_RX9+" direction="pas"/>
<pin name="PEG_RX9-" direction="pas"/>
<pin name="RSVD@9" direction="pas"/>
<pin name="GND@37" direction="pas"/>
<pin name="PEG_RX10+" direction="pas"/>
<pin name="PEG_RX10-" direction="pas"/>
<pin name="GND@38" direction="pas"/>
<pin name="PEG_RX11+" direction="pas"/>
<pin name="PEG_RX11-" direction="pas"/>
<pin name="GND@39" direction="pas"/>
<pin name="PEG_RX12+" direction="pas"/>
<pin name="PEG_RX12-" direction="pas"/>
<pin name="GND@40" direction="pas"/>
<pin name="PEG_RX13+" direction="pas"/>
<pin name="PEG_RX13-" direction="pas"/>
<pin name="GND@41" direction="pas"/>
<pin name="RSVD@10" direction="pas"/>
<pin name="PEG_RX14+" direction="pas"/>
<pin name="PEG_RX14-" direction="pas"/>
<pin name="GND@42" direction="pas"/>
<pin name="PEG_RX15+" direction="pas"/>
<pin name="PEG_RX15-" direction="pas"/>
<pin name="GND@43" direction="pas"/>
<pin name="VCC_12V@21" direction="pas"/>
<pin name="VCC_12V@22" direction="pas"/>
<pin name="VCC_12V@23" direction="pas"/>
<pin name="VCC_12V@24" direction="pas"/>
<pin name="VCC_12V@25" direction="pas"/>
<pin name="VCC_12V@26" direction="pas"/>
<pin name="GND@44" direction="pas"/>
<pin name="GND@45" direction="pas"/>
<pin name="IDE_D5" direction="pas"/>
<pin name="IDE_D10" direction="pas"/>
<pin name="IDE_D11" direction="pas"/>
<pin name="IDE_D12" direction="pas"/>
<pin name="IDE_D4" direction="pas"/>
<pin name="IDE_D0" direction="pas"/>
<pin name="IDE_REQ" direction="pas"/>
<pin name="!IDE_IOW" direction="pas"/>
<pin name="!IDE_ACK" direction="pas"/>
<pin name="GND@46" direction="pas"/>
<pin name="IDE_IRQ" direction="pas"/>
<pin name="IDE_A0" direction="pas"/>
<pin name="IDE_A1" direction="pas"/>
<pin name="IDE_A2" direction="pas"/>
<pin name="!IDE_CS1" direction="pas"/>
<pin name="!IDE_CS3" direction="pas"/>
<pin name="!IDE_RESET" direction="pas"/>
<pin name="!PCI_GNT3" direction="pas"/>
<pin name="!PCI_REQ3" direction="pas"/>
<pin name="GND@47" direction="pas"/>
<pin name="PCI_AD1" direction="pas"/>
<pin name="PCI_AD3" direction="pas"/>
<pin name="PCI_AD5" direction="pas"/>
<pin name="PCI_AD7" direction="pas"/>
<pin name="PCI_C/!BE0" direction="pas"/>
<pin name="PCI_AD9" direction="pas"/>
<pin name="PCI_AD11" direction="pas"/>
<pin name="PCI_AD13" direction="pas"/>
<pin name="PCI_AD15" direction="pas"/>
<pin name="GND@48" direction="pas"/>
<pin name="PCI_PAR" direction="pas"/>
<pin name="!PCI_SERR" direction="pas"/>
<pin name="!PCI_STOP" direction="pas"/>
<pin name="!PCI_TRDY" direction="pas"/>
<pin name="!PCI_FRAME" direction="pas"/>
<pin name="PCI_AD16" direction="pas"/>
<pin name="PCI_AD18" direction="pas"/>
<pin name="PCI_AD20" direction="pas"/>
<pin name="PCI_AD22" direction="pas"/>
<pin name="GND@49" direction="pas"/>
<pin name="PCI_AD24" direction="pas"/>
<pin name="PCI_AD26" direction="pas"/>
<pin name="PCI_AD28" direction="pas"/>
<pin name="PCI_AD30" direction="pas"/>
<pin name="!PCI_IRQC" direction="pas"/>
<pin name="!PCI_IRQD" direction="pas"/>
<pin name="!PCI_CLKRUN" direction="pas"/>
<pin name="PCI_M66EN" direction="pas"/>
<pin name="PCI_CLK" direction="pas"/>
<pin name="GND@50" direction="pas"/>
<pin name="PEG_TX0+" direction="pas"/>
<pin name="PEG_TX0-" direction="pas"/>
<pin name="!PEG_LANE_RV" direction="pas"/>
<pin name="PEG_TX1+" direction="pas"/>
<pin name="PEG_TX1-" direction="pas"/>
<pin name="!TYPE2" direction="pas"/>
<pin name="PEG_TX2+" direction="pas"/>
<pin name="PEG_TX2-" direction="pas"/>
<pin name="GND@51" direction="pas"/>
<pin name="PEG_TX3+" direction="pas"/>
<pin name="PEG_TX3-" direction="pas"/>
<pin name="RSVD@11" direction="pas"/>
<pin name="RSVD@12" direction="pas"/>
<pin name="PEG_TX4+" direction="pas"/>
<pin name="PEG_TX4-" direction="pas"/>
<pin name="GND@52" direction="pas"/>
<pin name="PEG_TX5+" direction="pas"/>
<pin name="PEG_TX5-" direction="pas"/>
<pin name="GND@53" direction="pas"/>
<pin name="PEG_TX6+" direction="pas"/>
<pin name="PEG_TX6-" direction="pas"/>
<pin name="SDVO_CLK" direction="pas"/>
<pin name="PEG_TX7+" direction="pas"/>
<pin name="PEG_TX7-" direction="pas"/>
<pin name="GND@54" direction="pas"/>
<pin name="IDE_CBLID" direction="pas"/>
<pin name="PEG_TX8+" direction="pas"/>
<pin name="PEG_TX8-" direction="pas"/>
<pin name="GND@55" direction="pas"/>
<pin name="PEG_TX9+" direction="pas"/>
<pin name="PEG_TX9-" direction="pas"/>
<pin name="RSVD@13" direction="pas"/>
<pin name="GND@56" direction="pas"/>
<pin name="PEG_TX10+" direction="pas"/>
<pin name="PEG_TX10-" direction="pas"/>
<pin name="GND@57" direction="pas"/>
<pin name="PEG_TX11+" direction="pas"/>
<pin name="PEG_TX11-" direction="pas"/>
<pin name="GND@58" direction="pas"/>
<pin name="PEG_TX12+" direction="pas"/>
<pin name="PEG_TX12-" direction="pas"/>
<pin name="GND@59" direction="pas"/>
<pin name="PEG_TX13+" direction="pas"/>
<pin name="PEG_TX13-" direction="pas"/>
<pin name="GND@60" direction="pas"/>
<pin name="!PEG_ENABLE" direction="pas"/>
<pin name="PEG_TX14+" direction="pas"/>
<pin name="PEG_TX14-" direction="pas"/>
<pin name="GND@61" direction="pas"/>
<pin name="PEG_TX15+" direction="pas"/>
<pin name="PEG_TX15-" direction="pas"/>
<pin name="GND@62" direction="pas"/>
<pin name="VCC_12V@27" direction="pas"/>
<pin name="VCC_12V@28" direction="pas"/>
<pin name="VCC_12V@29" direction="pas"/>
<pin name="VCC_12V@30" direction="pas"/>
<pin name="VCC_12V@31" direction="pas"/>
<pin name="VCC_12V@32" direction="pas"/>
<pin name="GND@63" direction="pas"/>
</symbol>
<symbol name="1PIN_NAME_VALUE">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="1PIN_NAME">
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ETX-X1" prefix="X">
<description>&lt;b&gt;PCI-Bus, USB, Audio&lt;/b&gt; ETX Board Connector 100 Pos.&lt;p&gt;
Source: www.kontron.com/techlib/whitepapers/etx_spec.pdf</description>
<gates>
<gate name="G$1" symbol="X1"/>
</gates>
<devices>
<device name="" package="FX8-100S-SV">
<connects>
<connect gate="G$1" pin="!CBE0" pad="31"/>
<connect gate="G$1" pin="!CBE1" pad="49"/>
<connect gate="G$1" pin="!CBE2" pad="70"/>
<connect gate="G$1" pin="!CBE3" pad="82"/>
<connect gate="G$1" pin="!DEVSEL" pad="60"/>
<connect gate="G$1" pin="!FRAME" pad="65"/>
<connect gate="G$1" pin="!GNT0" pad="17"/>
<connect gate="G$1" pin="!GNT1" pad="14"/>
<connect gate="G$1" pin="!GNT2" pad="11"/>
<connect gate="G$1" pin="!GNT3" pad="10"/>
<connect gate="G$1" pin="!GPERR" pad="55"/>
<connect gate="G$1" pin="!INTA" pad="97"/>
<connect gate="G$1" pin="!INTB" pad="98"/>
<connect gate="G$1" pin="!INTC" pad="95"/>
<connect gate="G$1" pin="!INTD" pad="96"/>
<connect gate="G$1" pin="!IRDY" pad="63"/>
<connect gate="G$1" pin="!LOCK" pad="59"/>
<connect gate="G$1" pin="!PCIRST" pad="93"/>
<connect gate="G$1" pin="!PME" pad="57"/>
<connect gate="G$1" pin="!REQ0" pad="22"/>
<connect gate="G$1" pin="!REQ1" pad="15"/>
<connect gate="G$1" pin="!REQ2" pad="13"/>
<connect gate="G$1" pin="!REQ3" pad="9"/>
<connect gate="G$1" pin="!SERR" pad="54"/>
<connect gate="G$1" pin="!STOP" pad="64"/>
<connect gate="G$1" pin="!TRDY" pad="61"/>
<connect gate="G$1" pin="!USB0" pad="76"/>
<connect gate="G$1" pin="!USB1" pad="80"/>
<connect gate="G$1" pin="!USB2" pad="58"/>
<connect gate="G$1" pin="!USB3" pad="62"/>
<connect gate="G$1" pin="3V" pad="12"/>
<connect gate="G$1" pin="3V@1" pad="16"/>
<connect gate="G$1" pin="3V@2" pad="24"/>
<connect gate="G$1" pin="AD0" pad="23"/>
<connect gate="G$1" pin="AD1" pad="25"/>
<connect gate="G$1" pin="AD10" pad="37"/>
<connect gate="G$1" pin="AD11" pad="39"/>
<connect gate="G$1" pin="AD12" pad="41"/>
<connect gate="G$1" pin="AD13" pad="43"/>
<connect gate="G$1" pin="AD14" pad="45"/>
<connect gate="G$1" pin="AD15" pad="47"/>
<connect gate="G$1" pin="AD16" pad="69"/>
<connect gate="G$1" pin="AD17" pad="71"/>
<connect gate="G$1" pin="AD18" pad="74"/>
<connect gate="G$1" pin="AD19" pad="73"/>
<connect gate="G$1" pin="AD2" pad="26"/>
<connect gate="G$1" pin="AD20" pad="75"/>
<connect gate="G$1" pin="AD21" pad="78"/>
<connect gate="G$1" pin="AD22" pad="77"/>
<connect gate="G$1" pin="AD23" pad="79"/>
<connect gate="G$1" pin="AD24" pad="81"/>
<connect gate="G$1" pin="AD25" pad="85"/>
<connect gate="G$1" pin="AD26" pad="86"/>
<connect gate="G$1" pin="AD27" pad="89"/>
<connect gate="G$1" pin="AD28" pad="87"/>
<connect gate="G$1" pin="AD29" pad="90"/>
<connect gate="G$1" pin="AD3" pad="28"/>
<connect gate="G$1" pin="AD30" pad="91"/>
<connect gate="G$1" pin="AD31" pad="94"/>
<connect gate="G$1" pin="AD4" pad="27"/>
<connect gate="G$1" pin="AD5" pad="30"/>
<connect gate="G$1" pin="AD6" pad="29"/>
<connect gate="G$1" pin="AD7" pad="32"/>
<connect gate="G$1" pin="AD8" pad="33"/>
<connect gate="G$1" pin="AD9" pad="34"/>
<connect gate="G$1" pin="ASGND" pad="48"/>
<connect gate="G$1" pin="ASVCC" pad="44"/>
<connect gate="G$1" pin="AUXAL" pad="38"/>
<connect gate="G$1" pin="AUXAR" pad="42"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="5"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="35"/>
<connect gate="G$1" pin="GND@5" pad="36"/>
<connect gate="G$1" pin="GND@6" pad="67"/>
<connect gate="G$1" pin="GND@7" pad="68"/>
<connect gate="G$1" pin="GND@8" pad="99"/>
<connect gate="G$1" pin="GND@9" pad="100"/>
<connect gate="G$1" pin="MIC" pad="40"/>
<connect gate="G$1" pin="PAR" pad="53"/>
<connect gate="G$1" pin="PCICLK1" pad="7"/>
<connect gate="G$1" pin="PCICLK2" pad="8"/>
<connect gate="G$1" pin="PCICLK3" pad="3"/>
<connect gate="G$1" pin="PCICLK4" pad="4"/>
<connect gate="G$1" pin="RESERVED" pad="18"/>
<connect gate="G$1" pin="RESERVED@1" pad="56"/>
<connect gate="G$1" pin="SERIRQ" pad="21"/>
<connect gate="G$1" pin="SNDL" pad="46"/>
<connect gate="G$1" pin="SNDR" pad="50"/>
<connect gate="G$1" pin="USB0" pad="88"/>
<connect gate="G$1" pin="USB1" pad="92"/>
<connect gate="G$1" pin="USB2" pad="66"/>
<connect gate="G$1" pin="USB3" pad="72"/>
<connect gate="G$1" pin="VCC" pad="19"/>
<connect gate="G$1" pin="VCC@1" pad="20"/>
<connect gate="G$1" pin="VCC@2" pad="51"/>
<connect gate="G$1" pin="VCC@3" pad="52"/>
<connect gate="G$1" pin="VCC@4" pad="83"/>
<connect gate="G$1" pin="VCC@5" pad="84"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ETX-X2" prefix="X">
<description>&lt;b&gt;ISA Bus&lt;/b&gt; ETX Board Connector 100 Pos.&lt;p&gt;
Source: www.kontron.com/techlib/whitepapers/etx_spec.pdf</description>
<gates>
<gate name="G$1" symbol="X2"/>
</gates>
<devices>
<device name="" package="FX8-100S-SV">
<connects>
<connect gate="G$1" pin="!DACK0" pad="22"/>
<connect gate="G$1" pin="!DACK1" pad="66"/>
<connect gate="G$1" pin="!DACK2" pad="46"/>
<connect gate="G$1" pin="!DACK3" pad="72"/>
<connect gate="G$1" pin="!DACK5" pad="18"/>
<connect gate="G$1" pin="!DACK6" pad="14"/>
<connect gate="G$1" pin="!DACK7" pad="10"/>
<connect gate="G$1" pin="!IO16" pad="34"/>
<connect gate="G$1" pin="!IOCHK" pad="97"/>
<connect gate="G$1" pin="!IOR" pad="74"/>
<connect gate="G$1" pin="!IOW" pad="76"/>
<connect gate="G$1" pin="!M16" pad="38"/>
<connect gate="G$1" pin="!MASTER" pad="6"/>
<connect gate="G$1" pin="!MEMR" pad="19"/>
<connect gate="G$1" pin="!MEMW" pad="17"/>
<connect gate="G$1" pin="!NOWS" pad="90"/>
<connect gate="G$1" pin="!REFSH" pad="62"/>
<connect gate="G$1" pin="!SBHE" pad="37"/>
<connect gate="G$1" pin="!SMEMR" pad="80"/>
<connect gate="G$1" pin="!SMEMW" pad="86"/>
<connect gate="G$1" pin="AEN" pad="82"/>
<connect gate="G$1" pin="BALE" pad="42"/>
<connect gate="G$1" pin="DREQ0" pad="20"/>
<connect gate="G$1" pin="DREQ1" pad="64"/>
<connect gate="G$1" pin="DREQ2" pad="91"/>
<connect gate="G$1" pin="DREQ3" pad="70"/>
<connect gate="G$1" pin="DREQ5" pad="16"/>
<connect gate="G$1" pin="DREQ6" pad="12"/>
<connect gate="G$1" pin="DREQ7" pad="8"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="35"/>
<connect gate="G$1" pin="GND@3" pad="36"/>
<connect gate="G$1" pin="GND@4" pad="67"/>
<connect gate="G$1" pin="GND@5" pad="68"/>
<connect gate="G$1" pin="GND@6" pad="99"/>
<connect gate="G$1" pin="GND@7" pad="100"/>
<connect gate="G$1" pin="IOCHRDY" pad="81"/>
<connect gate="G$1" pin="IRQ10" pad="32"/>
<connect gate="G$1" pin="IRQ11" pad="30"/>
<connect gate="G$1" pin="IRQ12" pad="28"/>
<connect gate="G$1" pin="IRQ14" pad="24"/>
<connect gate="G$1" pin="IRQ15" pad="26"/>
<connect gate="G$1" pin="IRQ3" pad="48"/>
<connect gate="G$1" pin="IRQ4" pad="50"/>
<connect gate="G$1" pin="IRQ5" pad="54"/>
<connect gate="G$1" pin="IRQ6" pad="56"/>
<connect gate="G$1" pin="IRQ7" pad="58"/>
<connect gate="G$1" pin="IRQ9" pad="94"/>
<connect gate="G$1" pin="LA17" pad="21"/>
<connect gate="G$1" pin="LA18" pad="23"/>
<connect gate="G$1" pin="LA19" pad="25"/>
<connect gate="G$1" pin="LA20" pad="27"/>
<connect gate="G$1" pin="LA21" pad="29"/>
<connect gate="G$1" pin="LA22" pad="31"/>
<connect gate="G$1" pin="LA23" pad="33"/>
<connect gate="G$1" pin="OSC" pad="40"/>
<connect gate="G$1" pin="RSTDRV" pad="98"/>
<connect gate="G$1" pin="SA0" pad="39"/>
<connect gate="G$1" pin="SA1" pad="41"/>
<connect gate="G$1" pin="SA10" pad="61"/>
<connect gate="G$1" pin="SA11" pad="63"/>
<connect gate="G$1" pin="SA12" pad="65"/>
<connect gate="G$1" pin="SA13" pad="69"/>
<connect gate="G$1" pin="SA14" pad="71"/>
<connect gate="G$1" pin="SA15" pad="73"/>
<connect gate="G$1" pin="SA16" pad="75"/>
<connect gate="G$1" pin="SA17" pad="78"/>
<connect gate="G$1" pin="SA18" pad="77"/>
<connect gate="G$1" pin="SA19" pad="79"/>
<connect gate="G$1" pin="SA2" pad="43"/>
<connect gate="G$1" pin="SA3" pad="45"/>
<connect gate="G$1" pin="SA4" pad="47"/>
<connect gate="G$1" pin="SA5" pad="49"/>
<connect gate="G$1" pin="SA6" pad="53"/>
<connect gate="G$1" pin="SA7" pad="55"/>
<connect gate="G$1" pin="SA8" pad="57"/>
<connect gate="G$1" pin="SA9" pad="59"/>
<connect gate="G$1" pin="SD0" pad="85"/>
<connect gate="G$1" pin="SD1" pad="88"/>
<connect gate="G$1" pin="SD10" pad="11"/>
<connect gate="G$1" pin="SD11" pad="9"/>
<connect gate="G$1" pin="SD12" pad="7"/>
<connect gate="G$1" pin="SD13" pad="5"/>
<connect gate="G$1" pin="SD14" pad="3"/>
<connect gate="G$1" pin="SD15" pad="4"/>
<connect gate="G$1" pin="SD2" pad="87"/>
<connect gate="G$1" pin="SD3" pad="89"/>
<connect gate="G$1" pin="SD4" pad="92"/>
<connect gate="G$1" pin="SD5" pad="93"/>
<connect gate="G$1" pin="SD6" pad="95"/>
<connect gate="G$1" pin="SD7" pad="96"/>
<connect gate="G$1" pin="SD8" pad="15"/>
<connect gate="G$1" pin="SD9" pad="13"/>
<connect gate="G$1" pin="SYSCLK" pad="60"/>
<connect gate="G$1" pin="TC" pad="44"/>
<connect gate="G$1" pin="VCC" pad="51"/>
<connect gate="G$1" pin="VCC@1" pad="52"/>
<connect gate="G$1" pin="VCC@2" pad="83"/>
<connect gate="G$1" pin="VCC@3" pad="84"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ETX-X3-ANALOG" prefix="X">
<description>&lt;b&gt;VGA, LCD, Video, COM1, COM2, LPT/Floppy, IrDA, Mouse, Keyboard&lt;/b&gt;&lt;p&gt;
PARALLEL INTERFACE PINOUT, FLOPPY SUPPORT MODE PINOUT&lt;br&gt;
ETX Board Connector 100 Pos.&lt;br&gt;
Source: www.kontron.com/techlib/whitepapers/etx_spec.pdf</description>
<gates>
<gate name="G$1" symbol="X3-ANALOG"/>
</gates>
<devices>
<device name="" package="FX8-100S-SV">
<connects>
<connect gate="G$1" pin="!ACK" pad="84"/>
<connect gate="G$1" pin="!AFD" pad="56"/>
<connect gate="G$1" pin="!BLON" pad="44"/>
<connect gate="G$1" pin="!CTS1" pad="93"/>
<connect gate="G$1" pin="!CTS2" pad="75"/>
<connect gate="G$1" pin="!DCD1" pad="89"/>
<connect gate="G$1" pin="!DCD2" pad="71"/>
<connect gate="G$1" pin="!DETECT" pad="9"/>
<connect gate="G$1" pin="!DIR" pad="64"/>
<connect gate="G$1" pin="!DSKCHG" pad="72"/>
<connect gate="G$1" pin="!DSR1" pad="91"/>
<connect gate="G$1" pin="!DSR2" pad="73"/>
<connect gate="G$1" pin="!DTR1" pad="87"/>
<connect gate="G$1" pin="!DTR2" pad="69"/>
<connect gate="G$1" pin="!ERR" pad="60"/>
<connect gate="G$1" pin="!INDEX" pad="80"/>
<connect gate="G$1" pin="!RI1" pad="97"/>
<connect gate="G$1" pin="!RI2" pad="79"/>
<connect gate="G$1" pin="!RTS1" pad="85"/>
<connect gate="G$1" pin="!RTS2" pad="67"/>
<connect gate="G$1" pin="!SLCT" pad="90"/>
<connect gate="G$1" pin="!SLIN" pad="70"/>
<connect gate="G$1" pin="B" pad="4"/>
<connect gate="G$1" pin="B0" pad="19"/>
<connect gate="G$1" pin="B1" pad="17"/>
<connect gate="G$1" pin="B2" pad="20"/>
<connect gate="G$1" pin="B3" pad="18"/>
<connect gate="G$1" pin="B4" pad="11"/>
<connect gate="G$1" pin="B5" pad="13"/>
<connect gate="G$1" pin="BIASON" pad="45"/>
<connect gate="G$1" pin="BUSY" pad="86"/>
<connect gate="G$1" pin="C" pad="50"/>
<connect gate="G$1" pin="COMP" pad="47"/>
<connect gate="G$1" pin="DDCK" pad="8"/>
<connect gate="G$1" pin="DDDA" pad="10"/>
<connect gate="G$1" pin="DIGON" pad="46"/>
<connect gate="G$1" pin="EN" pad="14"/>
<connect gate="G$1" pin="G" pad="6"/>
<connect gate="G$1" pin="G0" pad="32"/>
<connect gate="G$1" pin="G1" pad="30"/>
<connect gate="G$1" pin="G2" pad="23"/>
<connect gate="G$1" pin="G3" pad="25"/>
<connect gate="G$1" pin="G4" pad="26"/>
<connect gate="G$1" pin="G5" pad="24"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@10" pad="54"/>
<connect gate="G$1" pin="GND@11" pad="65"/>
<connect gate="G$1" pin="GND@12" pad="66"/>
<connect gate="G$1" pin="GND@13" pad="99"/>
<connect gate="G$1" pin="GND@14" pad="100"/>
<connect gate="G$1" pin="GND@2" pad="15"/>
<connect gate="G$1" pin="GND@3" pad="16"/>
<connect gate="G$1" pin="GND@4" pad="21"/>
<connect gate="G$1" pin="GND@5" pad="22"/>
<connect gate="G$1" pin="GND@6" pad="27"/>
<connect gate="G$1" pin="GND@7" pad="28"/>
<connect gate="G$1" pin="GND@8" pad="33"/>
<connect gate="G$1" pin="GND@9" pad="34"/>
<connect gate="G$1" pin="HSY" pad="5"/>
<connect gate="G$1" pin="IRRX" pad="59"/>
<connect gate="G$1" pin="IRTX" pad="61"/>
<connect gate="G$1" pin="JILI_CLK" pad="43"/>
<connect gate="G$1" pin="JILI_DAT" pad="41"/>
<connect gate="G$1" pin="KBCLK" pad="96"/>
<connect gate="G$1" pin="KBDAT" pad="98"/>
<connect gate="G$1" pin="LCDDO0" pad="37"/>
<connect gate="G$1" pin="LCDDO1" pad="35"/>
<connect gate="G$1" pin="LCDDO18" pad="12"/>
<connect gate="G$1" pin="LCDDO2" pad="38"/>
<connect gate="G$1" pin="LCDDO3" pad="36"/>
<connect gate="G$1" pin="LCDDO4" pad="29"/>
<connect gate="G$1" pin="LCDDO5" pad="31"/>
<connect gate="G$1" pin="LPT/!FLPY" pad="51"/>
<connect gate="G$1" pin="LTGIO0" pad="42"/>
<connect gate="G$1" pin="MSCLK" pad="92"/>
<connect gate="G$1" pin="MSDAT" pad="94"/>
<connect gate="G$1" pin="PD1" pad="78"/>
<connect gate="G$1" pin="PD2" pad="76"/>
<connect gate="G$1" pin="PD3" pad="74"/>
<connect gate="G$1" pin="PD5" pad="68"/>
<connect gate="G$1" pin="PD6" pad="62"/>
<connect gate="G$1" pin="PD7" pad="58"/>
<connect gate="G$1" pin="PE" pad="88"/>
<connect gate="G$1" pin="R" pad="3"/>
<connect gate="G$1" pin="RESERVED" pad="52"/>
<connect gate="G$1" pin="RESERVED@1" pad="55"/>
<connect gate="G$1" pin="RESERVED@2" pad="57"/>
<connect gate="G$1" pin="RXD1" pad="83"/>
<connect gate="G$1" pin="RXD2" pad="63"/>
<connect gate="G$1" pin="SYNC" pad="49"/>
<connect gate="G$1" pin="TXD1" pad="95"/>
<connect gate="G$1" pin="TXD2" pad="77"/>
<connect gate="G$1" pin="VCC" pad="39"/>
<connect gate="G$1" pin="VCC@1" pad="40"/>
<connect gate="G$1" pin="VCC@2" pad="53"/>
<connect gate="G$1" pin="VCC@3" pad="81"/>
<connect gate="G$1" pin="VCC@4" pad="82"/>
<connect gate="G$1" pin="VSY" pad="7"/>
<connect gate="G$1" pin="Y" pad="48"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ETX-X3-LVDS" prefix="X">
<description>&lt;b&gt;VGA, LCD, Video, COM1, COM2, LPT/Floppy, IrDA, Mouse, Keyboard&lt;/b&gt;&lt;p&gt;
LVDS INTERFACE PINOUT, PARALLEL PORT MODE PINOUT&lt;br&gt;
ETX Board Connector 100 Pos.&lt;br&gt;
Source: www.kontron.com/techlib/whitepapers/etx_spec.pdf</description>
<gates>
<gate name="G$1" symbol="X3-LVDS"/>
</gates>
<devices>
<device name="" package="FX8-100S-SV">
<connects>
<connect gate="G$1" pin="!BLON" pad="44"/>
<connect gate="G$1" pin="!CTS1" pad="93"/>
<connect gate="G$1" pin="!CTS2" pad="75"/>
<connect gate="G$1" pin="!DCD1" pad="89"/>
<connect gate="G$1" pin="!DCD2" pad="71"/>
<connect gate="G$1" pin="!DETECT" pad="9"/>
<connect gate="G$1" pin="!DSR1" pad="91"/>
<connect gate="G$1" pin="!DSR2" pad="73"/>
<connect gate="G$1" pin="!DTR1" pad="87"/>
<connect gate="G$1" pin="!DTR2" pad="69"/>
<connect gate="G$1" pin="!HDSEL" pad="60"/>
<connect gate="G$1" pin="!INIT" pad="64"/>
<connect gate="G$1" pin="!RDATA" pad="74"/>
<connect gate="G$1" pin="!RI1" pad="97"/>
<connect gate="G$1" pin="!RI2" pad="79"/>
<connect gate="G$1" pin="!RTS1" pad="85"/>
<connect gate="G$1" pin="!RTS2" pad="67"/>
<connect gate="G$1" pin="!STB" pad="55"/>
<connect gate="G$1" pin="!STEP" pad="70"/>
<connect gate="G$1" pin="!TRK0" pad="78"/>
<connect gate="G$1" pin="!WDATA" pad="88"/>
<connect gate="G$1" pin="!WGATE" pad="90"/>
<connect gate="G$1" pin="!WP" pad="76"/>
<connect gate="G$1" pin="B" pad="4"/>
<connect gate="G$1" pin="C" pad="50"/>
<connect gate="G$1" pin="COMP" pad="47"/>
<connect gate="G$1" pin="DDCK" pad="8"/>
<connect gate="G$1" pin="DDDA" pad="10"/>
<connect gate="G$1" pin="DENSEL" pad="56"/>
<connect gate="G$1" pin="DIGON" pad="46"/>
<connect gate="G$1" pin="DRV" pad="84"/>
<connect gate="G$1" pin="G" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@10" pad="54"/>
<connect gate="G$1" pin="GND@11" pad="65"/>
<connect gate="G$1" pin="GND@12" pad="66"/>
<connect gate="G$1" pin="GND@13" pad="99"/>
<connect gate="G$1" pin="GND@14" pad="100"/>
<connect gate="G$1" pin="GND@2" pad="15"/>
<connect gate="G$1" pin="GND@3" pad="16"/>
<connect gate="G$1" pin="GND@4" pad="21"/>
<connect gate="G$1" pin="GND@5" pad="22"/>
<connect gate="G$1" pin="GND@6" pad="27"/>
<connect gate="G$1" pin="GND@7" pad="28"/>
<connect gate="G$1" pin="GND@8" pad="33"/>
<connect gate="G$1" pin="GND@9" pad="34"/>
<connect gate="G$1" pin="HSY" pad="5"/>
<connect gate="G$1" pin="HSYNC" pad="45"/>
<connect gate="G$1" pin="IRRX" pad="59"/>
<connect gate="G$1" pin="IRTX" pad="61"/>
<connect gate="G$1" pin="JILI_CLK" pad="43"/>
<connect gate="G$1" pin="JILI_DAT" pad="41"/>
<connect gate="G$1" pin="KBCLK" pad="96"/>
<connect gate="G$1" pin="KBDAT" pad="98"/>
<connect gate="G$1" pin="LCDDO10" pad="26"/>
<connect gate="G$1" pin="LCDDO11" pad="24"/>
<connect gate="G$1" pin="LCDDO12" pad="19"/>
<connect gate="G$1" pin="LCDDO13" pad="17"/>
<connect gate="G$1" pin="LCDDO14" pad="20"/>
<connect gate="G$1" pin="LCDDO15" pad="18"/>
<connect gate="G$1" pin="LCDDO16" pad="11"/>
<connect gate="G$1" pin="LCDDO17" pad="13"/>
<connect gate="G$1" pin="LCDDO19" pad="14"/>
<connect gate="G$1" pin="LCDDO6" pad="32"/>
<connect gate="G$1" pin="LCDDO7" pad="30"/>
<connect gate="G$1" pin="LCDDO8" pad="23"/>
<connect gate="G$1" pin="LCDDO9" pad="25"/>
<connect gate="G$1" pin="LPT/!FLPY" pad="51"/>
<connect gate="G$1" pin="MOT" pad="86"/>
<connect gate="G$1" pin="MSCLK" pad="92"/>
<connect gate="G$1" pin="MSDAT" pad="94"/>
<connect gate="G$1" pin="PD0" pad="80"/>
<connect gate="G$1" pin="PD4" pad="72"/>
<connect gate="G$1" pin="R" pad="3"/>
<connect gate="G$1" pin="R0" pad="37"/>
<connect gate="G$1" pin="R1" pad="35"/>
<connect gate="G$1" pin="R2" pad="38"/>
<connect gate="G$1" pin="R3" pad="36"/>
<connect gate="G$1" pin="R4" pad="29"/>
<connect gate="G$1" pin="R5" pad="31"/>
<connect gate="G$1" pin="RESERVED" pad="52"/>
<connect gate="G$1" pin="RESERVED@1" pad="57"/>
<connect gate="G$1" pin="RESERVED@2" pad="58"/>
<connect gate="G$1" pin="RESERVED@3" pad="62"/>
<connect gate="G$1" pin="RESERVED@4" pad="68"/>
<connect gate="G$1" pin="RXD1" pad="83"/>
<connect gate="G$1" pin="RXD2" pad="63"/>
<connect gate="G$1" pin="SHFCLK" pad="12"/>
<connect gate="G$1" pin="SYNC" pad="49"/>
<connect gate="G$1" pin="TXD1" pad="95"/>
<connect gate="G$1" pin="TXD2" pad="77"/>
<connect gate="G$1" pin="VCC" pad="39"/>
<connect gate="G$1" pin="VCC@1" pad="40"/>
<connect gate="G$1" pin="VCC@2" pad="53"/>
<connect gate="G$1" pin="VCC@3" pad="81"/>
<connect gate="G$1" pin="VCC@4" pad="82"/>
<connect gate="G$1" pin="VSY" pad="7"/>
<connect gate="G$1" pin="VSYNC" pad="42"/>
<connect gate="G$1" pin="Y" pad="48"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ETX-X4" prefix="X">
<description>&lt;b&gt;IDE 1, IDE 2, Ethernet, Miscellaneous&lt;/b&gt; ETX Board Connector 100 Pos.&lt;p&gt;
Source: www.kontron.com/techlib/whitepapers/etx_spec.pdf</description>
<gates>
<gate name="G$1" symbol="X4"/>
</gates>
<devices>
<device name="" package="FX8-100S-SV">
<connects>
<connect gate="G$1" pin="!ACTLED" pad="12"/>
<connect gate="G$1" pin="!BATLOW" pad="41"/>
<connect gate="G$1" pin="!EXTSMI" pad="21"/>
<connect gate="G$1" pin="!GPCS" pad="20"/>
<connect gate="G$1" pin="!GPE1" pad="42"/>
<connect gate="G$1" pin="!GPE2" pad="89"/>
<connect gate="G$1" pin="!HDRST" pad="98"/>
<connect gate="G$1" pin="!KBINH" pad="9"/>
<connect gate="G$1" pin="!LILED" pad="10"/>
<connect gate="G$1" pin="!OVCR" pad="19"/>
<connect gate="G$1" pin="!PIDE_AK" pad="46"/>
<connect gate="G$1" pin="!PIDE_CS1" pad="32"/>
<connect gate="G$1" pin="!PIDE_CS3" pad="30"/>
<connect gate="G$1" pin="!PIDE_IOR" pad="52"/>
<connect gate="G$1" pin="!PIDE_IOW" pad="54"/>
<connect gate="G$1" pin="!PWRBTN" pad="7"/>
<connect gate="G$1" pin="!ROMKBCS" pad="13"/>
<connect gate="G$1" pin="!RSMRST" pad="11"/>
<connect gate="G$1" pin="!RXD" pad="91"/>
<connect gate="G$1" pin="!SIDE_AK" pad="43"/>
<connect gate="G$1" pin="!SIDE_CS1" pad="27"/>
<connect gate="G$1" pin="!SIDE_CS3" pad="25"/>
<connect gate="G$1" pin="!SIDE_IOR" pad="47"/>
<connect gate="G$1" pin="!SIDE_IOW" pad="51"/>
<connect gate="G$1" pin="!SMBALRT" pad="26"/>
<connect gate="G$1" pin="!SPEEDLED" pad="14"/>
<connect gate="G$1" pin="!TXD" pad="95"/>
<connect gate="G$1" pin="5V_SB" pad="3"/>
<connect gate="G$1" pin="BATT" pad="8"/>
<connect gate="G$1" pin="CBLID_P" pad="90"/>
<connect gate="G$1" pin="DASP_S" pad="28"/>
<connect gate="G$1" pin="EXT_PRG" pad="15"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="33"/>
<connect gate="G$1" pin="GND@3" pad="34"/>
<connect gate="G$1" pin="GND@4" pad="65"/>
<connect gate="G$1" pin="GND@5" pad="66"/>
<connect gate="G$1" pin="GND@6" pad="99"/>
<connect gate="G$1" pin="GND@7" pad="100"/>
<connect gate="G$1" pin="I2CLK" pad="16"/>
<connect gate="G$1" pin="I2DAT" pad="22"/>
<connect gate="G$1" pin="PDIAG_S" pad="35"/>
<connect gate="G$1" pin="PIDE_A0" pad="38"/>
<connect gate="G$1" pin="PIDE_A1" pad="40"/>
<connect gate="G$1" pin="PIDE_A2" pad="36"/>
<connect gate="G$1" pin="PIDE_D0" pad="60"/>
<connect gate="G$1" pin="PIDE_D1" pad="64"/>
<connect gate="G$1" pin="PIDE_D10" pad="80"/>
<connect gate="G$1" pin="PIDE_D11" pad="76"/>
<connect gate="G$1" pin="PIDE_D12" pad="72"/>
<connect gate="G$1" pin="PIDE_D13" pad="68"/>
<connect gate="G$1" pin="PIDE_D14" pad="62"/>
<connect gate="G$1" pin="PIDE_D15" pad="58"/>
<connect gate="G$1" pin="PIDE_D2" pad="70"/>
<connect gate="G$1" pin="PIDE_D3" pad="74"/>
<connect gate="G$1" pin="PIDE_D4" pad="78"/>
<connect gate="G$1" pin="PIDE_D5" pad="84"/>
<connect gate="G$1" pin="PIDE_D6" pad="88"/>
<connect gate="G$1" pin="PIDE_D7" pad="96"/>
<connect gate="G$1" pin="PIDE_D8" pad="92"/>
<connect gate="G$1" pin="PIDE_D9" pad="86"/>
<connect gate="G$1" pin="PIDE_DRQ" pad="56"/>
<connect gate="G$1" pin="PIDE_INTRQ" pad="44"/>
<connect gate="G$1" pin="PIDE_RDY" pad="48"/>
<connect gate="G$1" pin="PS_ON" pad="5"/>
<connect gate="G$1" pin="PWGIN" pad="4"/>
<connect gate="G$1" pin="RXD" pad="93"/>
<connect gate="G$1" pin="SIDE_A0" pad="31"/>
<connect gate="G$1" pin="SIDE_A1" pad="37"/>
<connect gate="G$1" pin="SIDE_A2" pad="29"/>
<connect gate="G$1" pin="SIDE_D0" pad="57"/>
<connect gate="G$1" pin="SIDE_D1" pad="61"/>
<connect gate="G$1" pin="SIDE_D10" pad="77"/>
<connect gate="G$1" pin="SIDE_D11" pad="73"/>
<connect gate="G$1" pin="SIDE_D12" pad="69"/>
<connect gate="G$1" pin="SIDE_D13" pad="63"/>
<connect gate="G$1" pin="SIDE_D14" pad="59"/>
<connect gate="G$1" pin="SIDE_D15" pad="55"/>
<connect gate="G$1" pin="SIDE_D2" pad="67"/>
<connect gate="G$1" pin="SIDE_D3" pad="71"/>
<connect gate="G$1" pin="SIDE_D4" pad="75"/>
<connect gate="G$1" pin="SIDE_D5" pad="79"/>
<connect gate="G$1" pin="SIDE_D6" pad="85"/>
<connect gate="G$1" pin="SIDE_D7" pad="94"/>
<connect gate="G$1" pin="SIDE_D8" pad="87"/>
<connect gate="G$1" pin="SIDE_D9" pad="83"/>
<connect gate="G$1" pin="SIDE_DRQ" pad="53"/>
<connect gate="G$1" pin="SIDE_INTRQ" pad="39"/>
<connect gate="G$1" pin="SIDE_RDY" pad="45"/>
<connect gate="G$1" pin="SMBCLK" pad="23"/>
<connect gate="G$1" pin="SMBDATA" pad="24"/>
<connect gate="G$1" pin="SPEAKER" pad="6"/>
<connect gate="G$1" pin="TXD" pad="97"/>
<connect gate="G$1" pin="VCC" pad="17"/>
<connect gate="G$1" pin="VCC@1" pad="18"/>
<connect gate="G$1" pin="VCC@2" pad="49"/>
<connect gate="G$1" pin="VCC@3" pad="50"/>
<connect gate="G$1" pin="VCC@4" pad="81"/>
<connect gate="G$1" pin="VCC@5" pad="82"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COMEXRESS" prefix="X">
<description>&lt;b&gt;ETX Express&lt;/b&gt; COM Express&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 27&lt;/i&gt;&lt;br&gt;
Source: http://catalog.tycoelectronics.com .. ENG_CS_889092_0.5mm_FH_Conn_0906.pdf&lt;br&gt;
http://nordic.kontron.com/searchresult/?searchterm=etxe_designguide_v1.4.pdf</description>
<gates>
<gate name="G$1" symbol="COMEXPRESS"/>
</gates>
<devices>
<device name="" package="C-5353652-36-3">
<connects>
<connect gate="G$1" pin="!AC_RST" pad="A30"/>
<connect gate="G$1" pin="!ATA_ACT" pad="A28"/>
<connect gate="G$1" pin="!BATLOW" pad="A27"/>
<connect gate="G$1" pin="!CB_RESET" pad="B50"/>
<connect gate="G$1" pin="!EXCD0_CPPE" pad="A49"/>
<connect gate="G$1" pin="!EXCD0_PERST" pad="A48"/>
<connect gate="G$1" pin="!EXCD1_CPPE" pad="B48"/>
<connect gate="G$1" pin="!EXCD1_PERST" pad="B47"/>
<connect gate="G$1" pin="!IDE_ACK" pad="D10"/>
<connect gate="G$1" pin="!IDE_CS1" pad="D16"/>
<connect gate="G$1" pin="!IDE_CS3" pad="D17"/>
<connect gate="G$1" pin="!IDE_IOR" pad="C14"/>
<connect gate="G$1" pin="!IDE_IOW" pad="D9"/>
<connect gate="G$1" pin="!IDE_RESET" pad="D18"/>
<connect gate="G$1" pin="!KBD_RST" pad="A86"/>
<connect gate="G$1" pin="!LPC_DRQ0" pad="B8"/>
<connect gate="G$1" pin="!PCI_CLKRUN" pad="D48"/>
<connect gate="G$1" pin="!PCI_DEVSEL" pad="C36"/>
<connect gate="G$1" pin="!PCI_FRAME" pad="D36"/>
<connect gate="G$1" pin="!PCI_GNT0" pad="C20"/>
<connect gate="G$1" pin="!PCI_GNT1" pad="C18"/>
<connect gate="G$1" pin="!PCI_GNT2" pad="C16"/>
<connect gate="G$1" pin="!PCI_GNT3" pad="D19"/>
<connect gate="G$1" pin="!PCI_IRDY" pad="C37"/>
<connect gate="G$1" pin="!PCI_IRQA" pad="C49"/>
<connect gate="G$1" pin="!PCI_IRQB" pad="C50"/>
<connect gate="G$1" pin="!PCI_IRQC" pad="D46"/>
<connect gate="G$1" pin="!PCI_IRQD" pad="D47"/>
<connect gate="G$1" pin="!PCI_LOCK" pad="C35"/>
<connect gate="G$1" pin="!PCI_PERR" pad="C34"/>
<connect gate="G$1" pin="!PCI_PME" pad="C15"/>
<connect gate="G$1" pin="!PCI_REQ0" pad="C22"/>
<connect gate="G$1" pin="!PCI_REQ1" pad="C19"/>
<connect gate="G$1" pin="!PCI_REQ2" pad="C17"/>
<connect gate="G$1" pin="!PCI_REQ3" pad="D20"/>
<connect gate="G$1" pin="!PCI_RST" pad="C23"/>
<connect gate="G$1" pin="!PCI_SERR" pad="D33"/>
<connect gate="G$1" pin="!PCI_STOP" pad="D34"/>
<connect gate="G$1" pin="!PCI_TRDY" pad="D35"/>
<connect gate="G$1" pin="!PEG_ENABLE" pad="D97"/>
<connect gate="G$1" pin="!PEG_LANE_RV" pad="D54"/>
<connect gate="G$1" pin="!PWRBTN" pad="B12"/>
<connect gate="G$1" pin="!SUS_S3" pad="A15"/>
<connect gate="G$1" pin="!SUS_S4" pad="A18"/>
<connect gate="G$1" pin="!SUS_S5" pad="A24"/>
<connect gate="G$1" pin="!SYS_RESET" pad="B49"/>
<connect gate="G$1" pin="!THRMTRIP" pad="A35"/>
<connect gate="G$1" pin="!TYPE0" pad="C54"/>
<connect gate="G$1" pin="!TYPE1" pad="C57"/>
<connect gate="G$1" pin="!TYPE2" pad="D57"/>
<connect gate="G$1" pin="!USB_0_1_OC" pad="B44"/>
<connect gate="G$1" pin="!USB_2_3_OC" pad="A44"/>
<connect gate="G$1" pin="!USB_4_5_OC" pad="B38"/>
<connect gate="G$1" pin="!USB_6_7_OC" pad="A38"/>
<connect gate="G$1" pin="!WAKE0" pad="B66"/>
<connect gate="G$1" pin="!WAKE1" pad="B67"/>
<connect gate="G$1" pin="AC_BITCLK" pad="A32"/>
<connect gate="G$1" pin="AC_SDIN0" pad="B30"/>
<connect gate="G$1" pin="AC_SDIN1" pad="B29"/>
<connect gate="G$1" pin="AC_SDIN2" pad="B28"/>
<connect gate="G$1" pin="AC_SDOUT" pad="A33"/>
<connect gate="G$1" pin="AC_SYNC" pad="A29"/>
<connect gate="G$1" pin="BIOS_DISABLE" pad="A34"/>
<connect gate="G$1" pin="GBE0_!LINK" pad="A8"/>
<connect gate="G$1" pin="GBE0_ACT" pad="B2"/>
<connect gate="G$1" pin="GBE0_CTREF" pad="A14"/>
<connect gate="G$1" pin="GBE0_LINK10" pad="A4"/>
<connect gate="G$1" pin="GBE0_LINK10@1" pad="A5"/>
<connect gate="G$1" pin="GBE0_MDI0+" pad="A13"/>
<connect gate="G$1" pin="GBE0_MDI0-" pad="A12"/>
<connect gate="G$1" pin="GBE0_MDI1+" pad="A10"/>
<connect gate="G$1" pin="GBE0_MDI1-" pad="A9"/>
<connect gate="G$1" pin="GBE0_MDI2+" pad="A7"/>
<connect gate="G$1" pin="GBE0_MDI2-" pad="A6"/>
<connect gate="G$1" pin="GBE0_MDI3+" pad="A3"/>
<connect gate="G$1" pin="GBE0_MDI3-" pad="A2"/>
<connect gate="G$1" pin="GND" pad="A1"/>
<connect gate="G$1" pin="GND@1" pad="A11"/>
<connect gate="G$1" pin="GND@10" pad="A80"/>
<connect gate="G$1" pin="GND@11" pad="A90"/>
<connect gate="G$1" pin="GND@12" pad="A96"/>
<connect gate="G$1" pin="GND@13" pad="A100"/>
<connect gate="G$1" pin="GND@14" pad="A110"/>
<connect gate="G$1" pin="GND@15" pad="B1"/>
<connect gate="G$1" pin="GND@16" pad="B11"/>
<connect gate="G$1" pin="GND@17" pad="B21"/>
<connect gate="G$1" pin="GND@18" pad="B31"/>
<connect gate="G$1" pin="GND@19" pad="B41"/>
<connect gate="G$1" pin="GND@2" pad="A21"/>
<connect gate="G$1" pin="GND@20" pad="B51"/>
<connect gate="G$1" pin="GND@21" pad="B60"/>
<connect gate="G$1" pin="GND@22" pad="B70"/>
<connect gate="G$1" pin="GND@23" pad="B80"/>
<connect gate="G$1" pin="GND@24" pad="B90"/>
<connect gate="G$1" pin="GND@25" pad="B100"/>
<connect gate="G$1" pin="GND@26" pad="B110"/>
<connect gate="G$1" pin="GND@27" pad="C1"/>
<connect gate="G$1" pin="GND@28" pad="C11"/>
<connect gate="G$1" pin="GND@29" pad="C21"/>
<connect gate="G$1" pin="GND@3" pad="A31"/>
<connect gate="G$1" pin="GND@30" pad="C31"/>
<connect gate="G$1" pin="GND@31" pad="C41"/>
<connect gate="G$1" pin="GND@32" pad="C51"/>
<connect gate="G$1" pin="GND@33" pad="C60"/>
<connect gate="G$1" pin="GND@34" pad="C70"/>
<connect gate="G$1" pin="GND@35" pad="C76"/>
<connect gate="G$1" pin="GND@36" pad="C80"/>
<connect gate="G$1" pin="GND@37" pad="C84"/>
<connect gate="G$1" pin="GND@38" pad="C87"/>
<connect gate="G$1" pin="GND@39" pad="C90"/>
<connect gate="G$1" pin="GND@4" pad="A41"/>
<connect gate="G$1" pin="GND@40" pad="C93"/>
<connect gate="G$1" pin="GND@41" pad="C96"/>
<connect gate="G$1" pin="GND@42" pad="C100"/>
<connect gate="G$1" pin="GND@43" pad="C103"/>
<connect gate="G$1" pin="GND@44" pad="C110"/>
<connect gate="G$1" pin="GND@45" pad="D1"/>
<connect gate="G$1" pin="GND@46" pad="D11"/>
<connect gate="G$1" pin="GND@47" pad="D21"/>
<connect gate="G$1" pin="GND@48" pad="D31"/>
<connect gate="G$1" pin="GND@49" pad="D41"/>
<connect gate="G$1" pin="GND@5" pad="A51"/>
<connect gate="G$1" pin="GND@50" pad="D51"/>
<connect gate="G$1" pin="GND@51" pad="D60"/>
<connect gate="G$1" pin="GND@52" pad="D67"/>
<connect gate="G$1" pin="GND@53" pad="D70"/>
<connect gate="G$1" pin="GND@54" pad="D76"/>
<connect gate="G$1" pin="GND@55" pad="D80"/>
<connect gate="G$1" pin="GND@56" pad="D84"/>
<connect gate="G$1" pin="GND@57" pad="D87"/>
<connect gate="G$1" pin="GND@58" pad="D90"/>
<connect gate="G$1" pin="GND@59" pad="D93"/>
<connect gate="G$1" pin="GND@6" pad="A57"/>
<connect gate="G$1" pin="GND@60" pad="D96"/>
<connect gate="G$1" pin="GND@61" pad="D100"/>
<connect gate="G$1" pin="GND@62" pad="D103"/>
<connect gate="G$1" pin="GND@63" pad="D110"/>
<connect gate="G$1" pin="GND@7" pad="A60"/>
<connect gate="G$1" pin="GND@8" pad="A66"/>
<connect gate="G$1" pin="GND@9" pad="A70"/>
<connect gate="G$1" pin="GPI0" pad="A54"/>
<connect gate="G$1" pin="GPI1" pad="A63"/>
<connect gate="G$1" pin="GPI2" pad="A67"/>
<connect gate="G$1" pin="GPI3" pad="A85"/>
<connect gate="G$1" pin="GPO0" pad="A93"/>
<connect gate="G$1" pin="GPO1" pad="B54"/>
<connect gate="G$1" pin="GPO2" pad="B57"/>
<connect gate="G$1" pin="GPO3" pad="B63"/>
<connect gate="G$1" pin="I2C_CK" pad="B33"/>
<connect gate="G$1" pin="I2C_DAT" pad="B34"/>
<connect gate="G$1" pin="IDE_A0" pad="D13"/>
<connect gate="G$1" pin="IDE_A1" pad="D14"/>
<connect gate="G$1" pin="IDE_A2" pad="D15"/>
<connect gate="G$1" pin="IDE_CBLID" pad="D77"/>
<connect gate="G$1" pin="IDE_D0" pad="D7"/>
<connect gate="G$1" pin="IDE_D1" pad="C10"/>
<connect gate="G$1" pin="IDE_D10" pad="D3"/>
<connect gate="G$1" pin="IDE_D11" pad="D4"/>
<connect gate="G$1" pin="IDE_D12" pad="D5"/>
<connect gate="G$1" pin="IDE_D13" pad="C9"/>
<connect gate="G$1" pin="IDE_D14" pad="C12"/>
<connect gate="G$1" pin="IDE_D15" pad="C5"/>
<connect gate="G$1" pin="IDE_D2" pad="C8"/>
<connect gate="G$1" pin="IDE_D3" pad="C4"/>
<connect gate="G$1" pin="IDE_D4" pad="D6"/>
<connect gate="G$1" pin="IDE_D5" pad="D2"/>
<connect gate="G$1" pin="IDE_D6" pad="C3"/>
<connect gate="G$1" pin="IDE_D7" pad="C2"/>
<connect gate="G$1" pin="IDE_D8" pad="C6"/>
<connect gate="G$1" pin="IDE_D9" pad="C7"/>
<connect gate="G$1" pin="IDE_IORDY" pad="C13"/>
<connect gate="G$1" pin="IDE_IRQ" pad="D12"/>
<connect gate="G$1" pin="IDE_REQ" pad="D8"/>
<connect gate="G$1" pin="KBD_A20GATE" pad="A87"/>
<connect gate="G$1" pin="LPC_AD0" pad="B4"/>
<connect gate="G$1" pin="LPC_AD1" pad="B5"/>
<connect gate="G$1" pin="LPC_AD2" pad="B6"/>
<connect gate="G$1" pin="LPC_AD3" pad="B7"/>
<connect gate="G$1" pin="LPC_CLK" pad="B10"/>
<connect gate="G$1" pin="LPC_DRQ1!" pad="B9"/>
<connect gate="G$1" pin="LPC_FRAME!" pad="B3"/>
<connect gate="G$1" pin="LPC_SERIRQ" pad="A50"/>
<connect gate="G$1" pin="LVDS_A0+" pad="A71"/>
<connect gate="G$1" pin="LVDS_A0-" pad="A72"/>
<connect gate="G$1" pin="LVDS_A1+" pad="A73"/>
<connect gate="G$1" pin="LVDS_A1-" pad="A74"/>
<connect gate="G$1" pin="LVDS_A2+" pad="A75"/>
<connect gate="G$1" pin="LVDS_A2-" pad="A76"/>
<connect gate="G$1" pin="LVDS_A3+" pad="A78"/>
<connect gate="G$1" pin="LVDS_A3-" pad="A79"/>
<connect gate="G$1" pin="LVDS_A_CK+" pad="A81"/>
<connect gate="G$1" pin="LVDS_A_CK-" pad="A82"/>
<connect gate="G$1" pin="LVDS_B0+" pad="B71"/>
<connect gate="G$1" pin="LVDS_B0-" pad="B72"/>
<connect gate="G$1" pin="LVDS_B1+" pad="B73"/>
<connect gate="G$1" pin="LVDS_B1-" pad="B74"/>
<connect gate="G$1" pin="LVDS_B2+" pad="B75"/>
<connect gate="G$1" pin="LVDS_B2-" pad="B76"/>
<connect gate="G$1" pin="LVDS_B3+" pad="B77"/>
<connect gate="G$1" pin="LVDS_B3-" pad="B78"/>
<connect gate="G$1" pin="LVDS_BKLT_CTRL" pad="B83"/>
<connect gate="G$1" pin="LVDS_BKLT_EN" pad="B79"/>
<connect gate="G$1" pin="LVDS_B_CK+" pad="B81"/>
<connect gate="G$1" pin="LVDS_B_CK-" pad="B82"/>
<connect gate="G$1" pin="LVDS_I2C_CK" pad="A83"/>
<connect gate="G$1" pin="LVDS_I2C_DAT" pad="A84"/>
<connect gate="G$1" pin="LVDS_VDD_EN" pad="A77"/>
<connect gate="G$1" pin="PCIE0_CK_REF+" pad="A88"/>
<connect gate="G$1" pin="PCIE0_CK_REF-" pad="A89"/>
<connect gate="G$1" pin="PCIE_RX0+" pad="B68"/>
<connect gate="G$1" pin="PCIE_RX0-" pad="B69"/>
<connect gate="G$1" pin="PCIE_RX1+" pad="B64"/>
<connect gate="G$1" pin="PCIE_RX1-" pad="B65"/>
<connect gate="G$1" pin="PCIE_RX2+" pad="B61"/>
<connect gate="G$1" pin="PCIE_RX2-" pad="B62"/>
<connect gate="G$1" pin="PCIE_RX3+" pad="B58"/>
<connect gate="G$1" pin="PCIE_RX3-" pad="B59"/>
<connect gate="G$1" pin="PCIE_RX4+" pad="B55"/>
<connect gate="G$1" pin="PCIE_RX4-" pad="B56"/>
<connect gate="G$1" pin="PCIE_RX5+" pad="B52"/>
<connect gate="G$1" pin="PCIE_RX5-" pad="B53"/>
<connect gate="G$1" pin="PCIE_TX0+" pad="A68"/>
<connect gate="G$1" pin="PCIE_TX0-" pad="A69"/>
<connect gate="G$1" pin="PCIE_TX1+" pad="A64"/>
<connect gate="G$1" pin="PCIE_TX1-" pad="A65"/>
<connect gate="G$1" pin="PCIE_TX2+" pad="A61"/>
<connect gate="G$1" pin="PCIE_TX2-" pad="A62"/>
<connect gate="G$1" pin="PCIE_TX3+" pad="A58"/>
<connect gate="G$1" pin="PCIE_TX3-" pad="A59"/>
<connect gate="G$1" pin="PCIE_TX4+" pad="A55"/>
<connect gate="G$1" pin="PCIE_TX4-" pad="A56"/>
<connect gate="G$1" pin="PCIE_TX5+" pad="A52"/>
<connect gate="G$1" pin="PCIE_TX5-" pad="A53"/>
<connect gate="G$1" pin="PCI_AD0" pad="C24"/>
<connect gate="G$1" pin="PCI_AD1" pad="D22"/>
<connect gate="G$1" pin="PCI_AD10" pad="C29"/>
<connect gate="G$1" pin="PCI_AD11" pad="D28"/>
<connect gate="G$1" pin="PCI_AD12" pad="C30"/>
<connect gate="G$1" pin="PCI_AD13" pad="D29"/>
<connect gate="G$1" pin="PCI_AD14" pad="C32"/>
<connect gate="G$1" pin="PCI_AD15" pad="D30"/>
<connect gate="G$1" pin="PCI_AD16" pad="D37"/>
<connect gate="G$1" pin="PCI_AD17" pad="C39"/>
<connect gate="G$1" pin="PCI_AD18" pad="D38"/>
<connect gate="G$1" pin="PCI_AD19" pad="C40"/>
<connect gate="G$1" pin="PCI_AD2" pad="C25"/>
<connect gate="G$1" pin="PCI_AD20" pad="D39"/>
<connect gate="G$1" pin="PCI_AD21" pad="C42"/>
<connect gate="G$1" pin="PCI_AD22" pad="D40"/>
<connect gate="G$1" pin="PCI_AD23" pad="C43"/>
<connect gate="G$1" pin="PCI_AD24" pad="D42"/>
<connect gate="G$1" pin="PCI_AD25" pad="C45"/>
<connect gate="G$1" pin="PCI_AD26" pad="D43"/>
<connect gate="G$1" pin="PCI_AD27" pad="C46"/>
<connect gate="G$1" pin="PCI_AD28" pad="D44"/>
<connect gate="G$1" pin="PCI_AD29" pad="C47"/>
<connect gate="G$1" pin="PCI_AD3" pad="D23"/>
<connect gate="G$1" pin="PCI_AD30" pad="D45"/>
<connect gate="G$1" pin="PCI_AD31" pad="C48"/>
<connect gate="G$1" pin="PCI_AD4" pad="C26"/>
<connect gate="G$1" pin="PCI_AD5" pad="D24"/>
<connect gate="G$1" pin="PCI_AD6" pad="C27"/>
<connect gate="G$1" pin="PCI_AD7" pad="D25"/>
<connect gate="G$1" pin="PCI_AD8" pad="C28"/>
<connect gate="G$1" pin="PCI_AD9" pad="D27"/>
<connect gate="G$1" pin="PCI_C/!BE0" pad="D26"/>
<connect gate="G$1" pin="PCI_C/!BE1" pad="C33"/>
<connect gate="G$1" pin="PCI_C/!BE2" pad="C38"/>
<connect gate="G$1" pin="PCI_C/!BE3" pad="C44"/>
<connect gate="G$1" pin="PCI_CLK" pad="D50"/>
<connect gate="G$1" pin="PCI_M66EN" pad="D49"/>
<connect gate="G$1" pin="PCI_PAR" pad="D32"/>
<connect gate="G$1" pin="PEG_RX0+" pad="C52"/>
<connect gate="G$1" pin="PEG_RX0-" pad="C53"/>
<connect gate="G$1" pin="PEG_RX1+" pad="C55"/>
<connect gate="G$1" pin="PEG_RX1-" pad="C56"/>
<connect gate="G$1" pin="PEG_RX10+" pad="C85"/>
<connect gate="G$1" pin="PEG_RX10-" pad="C86"/>
<connect gate="G$1" pin="PEG_RX11+" pad="C88"/>
<connect gate="G$1" pin="PEG_RX11-" pad="C89"/>
<connect gate="G$1" pin="PEG_RX12+" pad="C91"/>
<connect gate="G$1" pin="PEG_RX12-" pad="C92"/>
<connect gate="G$1" pin="PEG_RX13+" pad="C94"/>
<connect gate="G$1" pin="PEG_RX13-" pad="C95"/>
<connect gate="G$1" pin="PEG_RX14+" pad="C98"/>
<connect gate="G$1" pin="PEG_RX14-" pad="C99"/>
<connect gate="G$1" pin="PEG_RX15+" pad="C101"/>
<connect gate="G$1" pin="PEG_RX15-" pad="C102"/>
<connect gate="G$1" pin="PEG_RX2+" pad="C58"/>
<connect gate="G$1" pin="PEG_RX2-" pad="C59"/>
<connect gate="G$1" pin="PEG_RX3+" pad="C61"/>
<connect gate="G$1" pin="PEG_RX3-" pad="C62"/>
<connect gate="G$1" pin="PEG_RX4+" pad="C65"/>
<connect gate="G$1" pin="PEG_RX4-" pad="C66"/>
<connect gate="G$1" pin="PEG_RX5+" pad="C68"/>
<connect gate="G$1" pin="PEG_RX5-" pad="C69"/>
<connect gate="G$1" pin="PEG_RX6+" pad="C71"/>
<connect gate="G$1" pin="PEG_RX6-" pad="C72"/>
<connect gate="G$1" pin="PEG_RX7+" pad="C74"/>
<connect gate="G$1" pin="PEG_RX7-" pad="C75"/>
<connect gate="G$1" pin="PEG_RX8+" pad="C78"/>
<connect gate="G$1" pin="PEG_RX8-" pad="C79"/>
<connect gate="G$1" pin="PEG_RX9+" pad="C81"/>
<connect gate="G$1" pin="PEG_RX9-" pad="C82"/>
<connect gate="G$1" pin="PEG_TX0+" pad="D52"/>
<connect gate="G$1" pin="PEG_TX0-" pad="D53"/>
<connect gate="G$1" pin="PEG_TX1+" pad="D55"/>
<connect gate="G$1" pin="PEG_TX1-" pad="D56"/>
<connect gate="G$1" pin="PEG_TX10+" pad="D85"/>
<connect gate="G$1" pin="PEG_TX10-" pad="D86"/>
<connect gate="G$1" pin="PEG_TX11+" pad="D88"/>
<connect gate="G$1" pin="PEG_TX11-" pad="D89"/>
<connect gate="G$1" pin="PEG_TX12+" pad="D91"/>
<connect gate="G$1" pin="PEG_TX12-" pad="D92"/>
<connect gate="G$1" pin="PEG_TX13+" pad="D94"/>
<connect gate="G$1" pin="PEG_TX13-" pad="D95"/>
<connect gate="G$1" pin="PEG_TX14+" pad="D98"/>
<connect gate="G$1" pin="PEG_TX14-" pad="D99"/>
<connect gate="G$1" pin="PEG_TX15+" pad="D101"/>
<connect gate="G$1" pin="PEG_TX15-" pad="D102"/>
<connect gate="G$1" pin="PEG_TX2+" pad="D58"/>
<connect gate="G$1" pin="PEG_TX2-" pad="D59"/>
<connect gate="G$1" pin="PEG_TX3+" pad="D61"/>
<connect gate="G$1" pin="PEG_TX3-" pad="D62"/>
<connect gate="G$1" pin="PEG_TX4+" pad="D65"/>
<connect gate="G$1" pin="PEG_TX4-" pad="D66"/>
<connect gate="G$1" pin="PEG_TX5+" pad="D68"/>
<connect gate="G$1" pin="PEG_TX5-" pad="D69"/>
<connect gate="G$1" pin="PEG_TX6+" pad="D71"/>
<connect gate="G$1" pin="PEG_TX6-" pad="D72"/>
<connect gate="G$1" pin="PEG_TX7+" pad="D74"/>
<connect gate="G$1" pin="PEG_TX7-" pad="D75"/>
<connect gate="G$1" pin="PEG_TX8+" pad="D78"/>
<connect gate="G$1" pin="PEG_TX8-" pad="D79"/>
<connect gate="G$1" pin="PEG_TX9+" pad="D81"/>
<connect gate="G$1" pin="PEG_TX9-" pad="D82"/>
<connect gate="G$1" pin="PWR_OK" pad="B24"/>
<connect gate="G$1" pin="RSVD" pad="A91"/>
<connect gate="G$1" pin="RSVD@1" pad="A92"/>
<connect gate="G$1" pin="RSVD@10" pad="C97"/>
<connect gate="G$1" pin="RSVD@11" pad="D63"/>
<connect gate="G$1" pin="RSVD@12" pad="D64"/>
<connect gate="G$1" pin="RSVD@13" pad="D83"/>
<connect gate="G$1" pin="RSVD@2" pad="A94"/>
<connect gate="G$1" pin="RSVD@3" pad="A95"/>
<connect gate="G$1" pin="RSVD@4" pad="B88"/>
<connect gate="G$1" pin="RSVD@5" pad="C63"/>
<connect gate="G$1" pin="RSVD@6" pad="C64"/>
<connect gate="G$1" pin="RSVD@7" pad="C67"/>
<connect gate="G$1" pin="RSVD@8" pad="C77"/>
<connect gate="G$1" pin="RSVD@9" pad="C83"/>
<connect gate="G$1" pin="SATA0_RX+" pad="A19"/>
<connect gate="G$1" pin="SATA0_RX-" pad="A20"/>
<connect gate="G$1" pin="SATA0_TX+" pad="A16"/>
<connect gate="G$1" pin="SATA0_TX-" pad="A17"/>
<connect gate="G$1" pin="SATA1_RX+" pad="B19"/>
<connect gate="G$1" pin="SATA1_RX-" pad="B20"/>
<connect gate="G$1" pin="SATA1_TX+" pad="B16"/>
<connect gate="G$1" pin="SATA1_TX-" pad="B17"/>
<connect gate="G$1" pin="SATA2_RX+" pad="A25"/>
<connect gate="G$1" pin="SATA2_RX-" pad="A26"/>
<connect gate="G$1" pin="SATA2_TX+" pad="A22"/>
<connect gate="G$1" pin="SATA2_TX-" pad="A23"/>
<connect gate="G$1" pin="SATA3_RX+" pad="B25"/>
<connect gate="G$1" pin="SATA3_RX-" pad="B26"/>
<connect gate="G$1" pin="SATA3_TX+" pad="B22"/>
<connect gate="G$1" pin="SATA3_TX-" pad="B23"/>
<connect gate="G$1" pin="SDVO_CLK" pad="D73"/>
<connect gate="G$1" pin="SDVO_DATA" pad="C73"/>
<connect gate="G$1" pin="SMB_ALERT!" pad="B15"/>
<connect gate="G$1" pin="SMB_CK" pad="B13"/>
<connect gate="G$1" pin="SMB_DAT" pad="B14"/>
<connect gate="G$1" pin="SPKR" pad="B32"/>
<connect gate="G$1" pin="SUS_STAT!" pad="B18"/>
<connect gate="G$1" pin="THRM!" pad="B35"/>
<connect gate="G$1" pin="TV_DAC_A" pad="B97"/>
<connect gate="G$1" pin="TV_DAC_B" pad="B98"/>
<connect gate="G$1" pin="TV_DAC_C" pad="B99"/>
<connect gate="G$1" pin="USB0+" pad="A46"/>
<connect gate="G$1" pin="USB0-" pad="A45"/>
<connect gate="G$1" pin="USB1+" pad="B46"/>
<connect gate="G$1" pin="USB1-" pad="B45"/>
<connect gate="G$1" pin="USB2+" pad="A43"/>
<connect gate="G$1" pin="USB2-" pad="A42"/>
<connect gate="G$1" pin="USB3+" pad="B43"/>
<connect gate="G$1" pin="USB3-" pad="B42"/>
<connect gate="G$1" pin="USB4+" pad="A40"/>
<connect gate="G$1" pin="USB4-" pad="A39"/>
<connect gate="G$1" pin="USB5+" pad="B40"/>
<connect gate="G$1" pin="USB5-" pad="B39"/>
<connect gate="G$1" pin="USB6+" pad="A37"/>
<connect gate="G$1" pin="USB6-" pad="A36"/>
<connect gate="G$1" pin="USB7+" pad="B37"/>
<connect gate="G$1" pin="USB7-" pad="B36"/>
<connect gate="G$1" pin="VCC_12V" pad="A97"/>
<connect gate="G$1" pin="VCC_12V@1" pad="A98"/>
<connect gate="G$1" pin="VCC_12V@10" pad="A108"/>
<connect gate="G$1" pin="VCC_12V@11" pad="A109"/>
<connect gate="G$1" pin="VCC_12V@12" pad="B101"/>
<connect gate="G$1" pin="VCC_12V@13" pad="B102"/>
<connect gate="G$1" pin="VCC_12V@14" pad="B103"/>
<connect gate="G$1" pin="VCC_12V@15" pad="B104"/>
<connect gate="G$1" pin="VCC_12V@16" pad="B105"/>
<connect gate="G$1" pin="VCC_12V@17" pad="B106"/>
<connect gate="G$1" pin="VCC_12V@18" pad="B107"/>
<connect gate="G$1" pin="VCC_12V@19" pad="B108"/>
<connect gate="G$1" pin="VCC_12V@2" pad="A99"/>
<connect gate="G$1" pin="VCC_12V@20" pad="B109"/>
<connect gate="G$1" pin="VCC_12V@21" pad="C104"/>
<connect gate="G$1" pin="VCC_12V@22" pad="C105"/>
<connect gate="G$1" pin="VCC_12V@23" pad="C106"/>
<connect gate="G$1" pin="VCC_12V@24" pad="C107"/>
<connect gate="G$1" pin="VCC_12V@25" pad="C108"/>
<connect gate="G$1" pin="VCC_12V@26" pad="C109"/>
<connect gate="G$1" pin="VCC_12V@27" pad="D104"/>
<connect gate="G$1" pin="VCC_12V@28" pad="D105"/>
<connect gate="G$1" pin="VCC_12V@29" pad="D106"/>
<connect gate="G$1" pin="VCC_12V@3" pad="A101"/>
<connect gate="G$1" pin="VCC_12V@30" pad="D107"/>
<connect gate="G$1" pin="VCC_12V@31" pad="D108"/>
<connect gate="G$1" pin="VCC_12V@32" pad="D109"/>
<connect gate="G$1" pin="VCC_12V@4" pad="A102"/>
<connect gate="G$1" pin="VCC_12V@5" pad="A103"/>
<connect gate="G$1" pin="VCC_12V@6" pad="A104"/>
<connect gate="G$1" pin="VCC_12V@7" pad="A105"/>
<connect gate="G$1" pin="VCC_12V@8" pad="A106"/>
<connect gate="G$1" pin="VCC_12V@9" pad="A107"/>
<connect gate="G$1" pin="VCC_5V_SBY" pad="B84"/>
<connect gate="G$1" pin="VCC_5V_SBY@1" pad="B85"/>
<connect gate="G$1" pin="VCC_5V_SBY@2" pad="B86"/>
<connect gate="G$1" pin="VCC_5V_SBY@3" pad="B87"/>
<connect gate="G$1" pin="VCC_RTC" pad="A47"/>
<connect gate="G$1" pin="VGA_BLU" pad="B92"/>
<connect gate="G$1" pin="VGA_GRN" pad="B91"/>
<connect gate="G$1" pin="VGA_HSYNC" pad="B93"/>
<connect gate="G$1" pin="VGA_I2C_CK" pad="B95"/>
<connect gate="G$1" pin="VGA_I2C_DAT" pad="B96"/>
<connect gate="G$1" pin="VGA_RED" pad="B89"/>
<connect gate="G$1" pin="VGA_VSYNC" pad="B94"/>
<connect gate="G$1" pin="WDT" pad="B27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="COMEXPRESS_S" prefix="X">
<description>&lt;b&gt;ETX Express&lt;/b&gt; COM Express&lt;p&gt;
Device generated with &lt;i&gt;split-gate-in-device-to-single-gates.ulp&lt;/i&gt; from &lt;b&gt;C-5353652-36-3.dev&lt;/b&gt;&lt;p&gt;
at 04.12.08 14:01:30 with EAGLE Version 5.3.5 Copyright (c) 1988-2008 CadSoft&lt;br&gt;
Source: http://catalog.tycoelectronics.com .. ENG_CS_889092_0.5mm_FH_Conn_0906.pdf&lt;br&gt;
http://nordic.kontron.com/searchresult/?searchterm=etxe_designguide_v1.4.pdf</description>
<gates>
<gate name="-GND" symbol="1PIN_NAME_VALUE"/>
<gate name="-GBE0_MDI3-" symbol="1PIN_NAME"/>
<gate name="-GBE0_MDI3+" symbol="1PIN_NAME"/>
<gate name="-GBE0_LINK10" symbol="1PIN_NAME"/>
<gate name="-GBE0_LINK10@1" symbol="1PIN_NAME"/>
<gate name="-GBE0_MDI2-" symbol="1PIN_NAME"/>
<gate name="-GBE0_MDI2+" symbol="1PIN_NAME"/>
<gate name="-GBE0_!LINK" symbol="1PIN_NAME"/>
<gate name="-GBE0_MDI1-" symbol="1PIN_NAME"/>
<gate name="-GBE0_MDI1+" symbol="1PIN_NAME"/>
<gate name="-GND@1" symbol="1PIN_NAME"/>
<gate name="-GBE0_MDI0-" symbol="1PIN_NAME"/>
<gate name="-GBE0_MDI0+" symbol="1PIN_NAME"/>
<gate name="-GBE0_CTREF" symbol="1PIN_NAME"/>
<gate name="-!SUS_S3" symbol="1PIN_NAME"/>
<gate name="-SATA0_TX+" symbol="1PIN_NAME"/>
<gate name="-SATA0_TX-" symbol="1PIN_NAME"/>
<gate name="-!SUS_S4" symbol="1PIN_NAME"/>
<gate name="-SATA0_RX+" symbol="1PIN_NAME"/>
<gate name="-SATA0_RX-" symbol="1PIN_NAME"/>
<gate name="-GND@2" symbol="1PIN_NAME"/>
<gate name="-SATA2_TX+" symbol="1PIN_NAME"/>
<gate name="-SATA2_TX-" symbol="1PIN_NAME"/>
<gate name="-!SUS_S5" symbol="1PIN_NAME"/>
<gate name="-SATA2_RX+" symbol="1PIN_NAME"/>
<gate name="-SATA2_RX-" symbol="1PIN_NAME"/>
<gate name="-!BATLOW" symbol="1PIN_NAME"/>
<gate name="-!ATA_ACT" symbol="1PIN_NAME"/>
<gate name="-AC_SYNC" symbol="1PIN_NAME"/>
<gate name="-!AC_RST" symbol="1PIN_NAME"/>
<gate name="-GND@3" symbol="1PIN_NAME"/>
<gate name="-AC_BITCLK" symbol="1PIN_NAME"/>
<gate name="-AC_SDOUT" symbol="1PIN_NAME"/>
<gate name="-BIOS_DISABLE" symbol="1PIN_NAME"/>
<gate name="-!THRMTRIP" symbol="1PIN_NAME"/>
<gate name="-USB6-" symbol="1PIN_NAME"/>
<gate name="-USB6+" symbol="1PIN_NAME"/>
<gate name="-!USB_6_7_OC" symbol="1PIN_NAME"/>
<gate name="-USB4-" symbol="1PIN_NAME"/>
<gate name="-USB4+" symbol="1PIN_NAME"/>
<gate name="-GND@4" symbol="1PIN_NAME"/>
<gate name="-USB2-" symbol="1PIN_NAME"/>
<gate name="-USB2+" symbol="1PIN_NAME"/>
<gate name="-!USB_2_3_OC" symbol="1PIN_NAME"/>
<gate name="-USB0-" symbol="1PIN_NAME"/>
<gate name="-USB0+" symbol="1PIN_NAME"/>
<gate name="-VCC_RTC" symbol="1PIN_NAME"/>
<gate name="-!EXCD0_PERST" symbol="1PIN_NAME"/>
<gate name="-!EXCD0_CPPE" symbol="1PIN_NAME"/>
<gate name="-LPC_SERIRQ" symbol="1PIN_NAME"/>
<gate name="-GND@5" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX5+" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX5-" symbol="1PIN_NAME"/>
<gate name="-GPI0" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX4+" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX4-" symbol="1PIN_NAME"/>
<gate name="-GND@6" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX3+" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX3-" symbol="1PIN_NAME"/>
<gate name="-GND@7" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX2+" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX2-" symbol="1PIN_NAME"/>
<gate name="-GPI1" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX1+" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX1-" symbol="1PIN_NAME"/>
<gate name="-GND@8" symbol="1PIN_NAME"/>
<gate name="-GPI2" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX0+" symbol="1PIN_NAME"/>
<gate name="-PCIE_TX0-" symbol="1PIN_NAME"/>
<gate name="-GND@9" symbol="1PIN_NAME"/>
<gate name="-LVDS_A0+" symbol="1PIN_NAME"/>
<gate name="-LVDS_A0-" symbol="1PIN_NAME"/>
<gate name="-LVDS_A1+" symbol="1PIN_NAME"/>
<gate name="-LVDS_A1-" symbol="1PIN_NAME"/>
<gate name="-LVDS_A2+" symbol="1PIN_NAME"/>
<gate name="-LVDS_A2-" symbol="1PIN_NAME"/>
<gate name="-LVDS_VDD_EN" symbol="1PIN_NAME"/>
<gate name="-LVDS_A3+" symbol="1PIN_NAME"/>
<gate name="-LVDS_A3-" symbol="1PIN_NAME"/>
<gate name="-GND@10" symbol="1PIN_NAME"/>
<gate name="-LVDS_A_CK+" symbol="1PIN_NAME"/>
<gate name="-LVDS_A_CK-" symbol="1PIN_NAME"/>
<gate name="-LVDS_I2C_CK" symbol="1PIN_NAME"/>
<gate name="-LVDS_I2C_DAT" symbol="1PIN_NAME"/>
<gate name="-GPI3" symbol="1PIN_NAME"/>
<gate name="-!KBD_RST" symbol="1PIN_NAME"/>
<gate name="-KBD_A20GATE" symbol="1PIN_NAME"/>
<gate name="-PCIE0_CK_REF+" symbol="1PIN_NAME"/>
<gate name="-PCIE0_CK_REF-" symbol="1PIN_NAME"/>
<gate name="-GND@11" symbol="1PIN_NAME"/>
<gate name="-RSVD" symbol="1PIN_NAME"/>
<gate name="-RSVD@1" symbol="1PIN_NAME"/>
<gate name="-GPO0" symbol="1PIN_NAME"/>
<gate name="-RSVD@2" symbol="1PIN_NAME"/>
<gate name="-RSVD@3" symbol="1PIN_NAME"/>
<gate name="-GND@12" symbol="1PIN_NAME"/>
<gate name="-VCC_12V" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@1" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@2" symbol="1PIN_NAME"/>
<gate name="-GND@13" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@3" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@4" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@5" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@6" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@7" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@8" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@9" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@10" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@11" symbol="1PIN_NAME"/>
<gate name="-GND@14" symbol="1PIN_NAME"/>
<gate name="-GND@15" symbol="1PIN_NAME"/>
<gate name="-GBE0_ACT" symbol="1PIN_NAME"/>
<gate name="-LPC_FRAME!" symbol="1PIN_NAME"/>
<gate name="-LPC_AD0" symbol="1PIN_NAME"/>
<gate name="-LPC_AD1" symbol="1PIN_NAME"/>
<gate name="-LPC_AD2" symbol="1PIN_NAME"/>
<gate name="-LPC_AD3" symbol="1PIN_NAME"/>
<gate name="-!LPC_DRQ0" symbol="1PIN_NAME"/>
<gate name="-LPC_DRQ1!" symbol="1PIN_NAME"/>
<gate name="-LPC_CLK" symbol="1PIN_NAME"/>
<gate name="-GND@16" symbol="1PIN_NAME"/>
<gate name="-!PWRBTN" symbol="1PIN_NAME"/>
<gate name="-SMB_CK" symbol="1PIN_NAME"/>
<gate name="-SMB_DAT" symbol="1PIN_NAME"/>
<gate name="-SMB_ALERT!" symbol="1PIN_NAME"/>
<gate name="-SATA1_TX+" symbol="1PIN_NAME"/>
<gate name="-SATA1_TX-" symbol="1PIN_NAME"/>
<gate name="-SUS_STAT!" symbol="1PIN_NAME"/>
<gate name="-SATA1_RX+" symbol="1PIN_NAME"/>
<gate name="-SATA1_RX-" symbol="1PIN_NAME"/>
<gate name="-GND@17" symbol="1PIN_NAME"/>
<gate name="-SATA3_TX+" symbol="1PIN_NAME"/>
<gate name="-SATA3_TX-" symbol="1PIN_NAME"/>
<gate name="-PWR_OK" symbol="1PIN_NAME"/>
<gate name="-SATA3_RX+" symbol="1PIN_NAME"/>
<gate name="-SATA3_RX-" symbol="1PIN_NAME"/>
<gate name="-WDT" symbol="1PIN_NAME"/>
<gate name="-AC_SDIN2" symbol="1PIN_NAME"/>
<gate name="-AC_SDIN1" symbol="1PIN_NAME"/>
<gate name="-AC_SDIN0" symbol="1PIN_NAME"/>
<gate name="-GND@18" symbol="1PIN_NAME"/>
<gate name="-SPKR" symbol="1PIN_NAME"/>
<gate name="-I2C_CK" symbol="1PIN_NAME"/>
<gate name="-I2C_DAT" symbol="1PIN_NAME"/>
<gate name="-THRM!" symbol="1PIN_NAME"/>
<gate name="-USB7-" symbol="1PIN_NAME"/>
<gate name="-USB7+" symbol="1PIN_NAME"/>
<gate name="-!USB_4_5_OC" symbol="1PIN_NAME"/>
<gate name="-USB5-" symbol="1PIN_NAME"/>
<gate name="-USB5+" symbol="1PIN_NAME"/>
<gate name="-GND@19" symbol="1PIN_NAME"/>
<gate name="-USB3-" symbol="1PIN_NAME"/>
<gate name="-USB3+" symbol="1PIN_NAME"/>
<gate name="-!USB_0_1_OC" symbol="1PIN_NAME"/>
<gate name="-USB1-" symbol="1PIN_NAME"/>
<gate name="-USB1+" symbol="1PIN_NAME"/>
<gate name="-!EXCD1_PERST" symbol="1PIN_NAME"/>
<gate name="-!EXCD1_CPPE" symbol="1PIN_NAME"/>
<gate name="-!SYS_RESET" symbol="1PIN_NAME"/>
<gate name="-!CB_RESET" symbol="1PIN_NAME"/>
<gate name="-GND@20" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX5+" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX5-" symbol="1PIN_NAME"/>
<gate name="-GPO1" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX4+" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX4-" symbol="1PIN_NAME"/>
<gate name="-GPO2" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX3+" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX3-" symbol="1PIN_NAME"/>
<gate name="-GND@21" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX2+" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX2-" symbol="1PIN_NAME"/>
<gate name="-GPO3" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX1+" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX1-" symbol="1PIN_NAME"/>
<gate name="-!WAKE0" symbol="1PIN_NAME"/>
<gate name="-!WAKE1" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX0+" symbol="1PIN_NAME"/>
<gate name="-PCIE_RX0-" symbol="1PIN_NAME"/>
<gate name="-GND@22" symbol="1PIN_NAME"/>
<gate name="-LVDS_B0+" symbol="1PIN_NAME"/>
<gate name="-LVDS_B0-" symbol="1PIN_NAME"/>
<gate name="-LVDS_B1+" symbol="1PIN_NAME"/>
<gate name="-LVDS_B1-" symbol="1PIN_NAME"/>
<gate name="-LVDS_B2+" symbol="1PIN_NAME"/>
<gate name="-LVDS_B2-" symbol="1PIN_NAME"/>
<gate name="-LVDS_B3+" symbol="1PIN_NAME"/>
<gate name="-LVDS_B3-" symbol="1PIN_NAME"/>
<gate name="-LVDS_BKLT_EN" symbol="1PIN_NAME"/>
<gate name="-GND@23" symbol="1PIN_NAME"/>
<gate name="-LVDS_B_CK+" symbol="1PIN_NAME"/>
<gate name="-LVDS_B_CK-" symbol="1PIN_NAME"/>
<gate name="-LVDS_BKLT_CTRL" symbol="1PIN_NAME"/>
<gate name="-VCC_5V_SBY" symbol="1PIN_NAME"/>
<gate name="-VCC_5V_SBY@1" symbol="1PIN_NAME"/>
<gate name="-VCC_5V_SBY@2" symbol="1PIN_NAME"/>
<gate name="-VCC_5V_SBY@3" symbol="1PIN_NAME"/>
<gate name="-RSVD@4" symbol="1PIN_NAME"/>
<gate name="-VGA_RED" symbol="1PIN_NAME"/>
<gate name="-GND@24" symbol="1PIN_NAME"/>
<gate name="-VGA_GRN" symbol="1PIN_NAME"/>
<gate name="-VGA_BLU" symbol="1PIN_NAME"/>
<gate name="-VGA_HSYNC" symbol="1PIN_NAME"/>
<gate name="-VGA_VSYNC" symbol="1PIN_NAME"/>
<gate name="-VGA_I2C_CK" symbol="1PIN_NAME"/>
<gate name="-VGA_I2C_DAT" symbol="1PIN_NAME"/>
<gate name="-TV_DAC_A" symbol="1PIN_NAME"/>
<gate name="-TV_DAC_B" symbol="1PIN_NAME"/>
<gate name="-TV_DAC_C" symbol="1PIN_NAME"/>
<gate name="-GND@25" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@12" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@13" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@14" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@15" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@16" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@17" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@18" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@19" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@20" symbol="1PIN_NAME"/>
<gate name="-GND@26" symbol="1PIN_NAME"/>
<gate name="-GND@27" symbol="1PIN_NAME"/>
<gate name="-IDE_D7" symbol="1PIN_NAME"/>
<gate name="-IDE_D6" symbol="1PIN_NAME"/>
<gate name="-IDE_D3" symbol="1PIN_NAME"/>
<gate name="-IDE_D15" symbol="1PIN_NAME"/>
<gate name="-IDE_D8" symbol="1PIN_NAME"/>
<gate name="-IDE_D9" symbol="1PIN_NAME"/>
<gate name="-IDE_D2" symbol="1PIN_NAME"/>
<gate name="-IDE_D13" symbol="1PIN_NAME"/>
<gate name="-IDE_D1" symbol="1PIN_NAME"/>
<gate name="-GND@28" symbol="1PIN_NAME"/>
<gate name="-IDE_D14" symbol="1PIN_NAME"/>
<gate name="-IDE_IORDY" symbol="1PIN_NAME"/>
<gate name="-!IDE_IOR" symbol="1PIN_NAME"/>
<gate name="-!PCI_PME" symbol="1PIN_NAME"/>
<gate name="-!PCI_GNT2" symbol="1PIN_NAME"/>
<gate name="-!PCI_REQ2" symbol="1PIN_NAME"/>
<gate name="-!PCI_GNT1" symbol="1PIN_NAME"/>
<gate name="-!PCI_REQ1" symbol="1PIN_NAME"/>
<gate name="-!PCI_GNT0" symbol="1PIN_NAME"/>
<gate name="-GND@29" symbol="1PIN_NAME"/>
<gate name="-!PCI_REQ0" symbol="1PIN_NAME"/>
<gate name="-!PCI_RST" symbol="1PIN_NAME"/>
<gate name="-PCI_AD0" symbol="1PIN_NAME"/>
<gate name="-PCI_AD2" symbol="1PIN_NAME"/>
<gate name="-PCI_AD4" symbol="1PIN_NAME"/>
<gate name="-PCI_AD6" symbol="1PIN_NAME"/>
<gate name="-PCI_AD8" symbol="1PIN_NAME"/>
<gate name="-PCI_AD10" symbol="1PIN_NAME"/>
<gate name="-PCI_AD12" symbol="1PIN_NAME"/>
<gate name="-GND@30" symbol="1PIN_NAME"/>
<gate name="-PCI_AD14" symbol="1PIN_NAME"/>
<gate name="-PCI_C/!BE1" symbol="1PIN_NAME"/>
<gate name="-!PCI_PERR" symbol="1PIN_NAME"/>
<gate name="-!PCI_LOCK" symbol="1PIN_NAME"/>
<gate name="-!PCI_DEVSEL" symbol="1PIN_NAME"/>
<gate name="-!PCI_IRDY" symbol="1PIN_NAME"/>
<gate name="-PCI_C/!BE2" symbol="1PIN_NAME"/>
<gate name="-PCI_AD17" symbol="1PIN_NAME"/>
<gate name="-PCI_AD19" symbol="1PIN_NAME"/>
<gate name="-GND@31" symbol="1PIN_NAME"/>
<gate name="-PCI_AD21" symbol="1PIN_NAME"/>
<gate name="-PCI_AD23" symbol="1PIN_NAME"/>
<gate name="-PCI_C/!BE3" symbol="1PIN_NAME"/>
<gate name="-PCI_AD25" symbol="1PIN_NAME"/>
<gate name="-PCI_AD27" symbol="1PIN_NAME"/>
<gate name="-PCI_AD29" symbol="1PIN_NAME"/>
<gate name="-PCI_AD31" symbol="1PIN_NAME"/>
<gate name="-!PCI_IRQA" symbol="1PIN_NAME"/>
<gate name="-!PCI_IRQB" symbol="1PIN_NAME"/>
<gate name="-GND@32" symbol="1PIN_NAME"/>
<gate name="-PEG_RX0+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX0-" symbol="1PIN_NAME"/>
<gate name="-!TYPE0" symbol="1PIN_NAME"/>
<gate name="-PEG_RX1+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX1-" symbol="1PIN_NAME"/>
<gate name="-!TYPE1" symbol="1PIN_NAME"/>
<gate name="-PEG_RX2+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX2-" symbol="1PIN_NAME"/>
<gate name="-GND@33" symbol="1PIN_NAME"/>
<gate name="-PEG_RX3+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX3-" symbol="1PIN_NAME"/>
<gate name="-RSVD@5" symbol="1PIN_NAME"/>
<gate name="-RSVD@6" symbol="1PIN_NAME"/>
<gate name="-PEG_RX4+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX4-" symbol="1PIN_NAME"/>
<gate name="-RSVD@7" symbol="1PIN_NAME"/>
<gate name="-PEG_RX5+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX5-" symbol="1PIN_NAME"/>
<gate name="-GND@34" symbol="1PIN_NAME"/>
<gate name="-PEG_RX6+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX6-" symbol="1PIN_NAME"/>
<gate name="-SDVO_DATA" symbol="1PIN_NAME"/>
<gate name="-PEG_RX7+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX7-" symbol="1PIN_NAME"/>
<gate name="-GND@35" symbol="1PIN_NAME"/>
<gate name="-RSVD@8" symbol="1PIN_NAME"/>
<gate name="-PEG_RX8+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX8-" symbol="1PIN_NAME"/>
<gate name="-GND@36" symbol="1PIN_NAME"/>
<gate name="-PEG_RX9+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX9-" symbol="1PIN_NAME"/>
<gate name="-RSVD@9" symbol="1PIN_NAME"/>
<gate name="-GND@37" symbol="1PIN_NAME"/>
<gate name="-PEG_RX10+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX10-" symbol="1PIN_NAME"/>
<gate name="-GND@38" symbol="1PIN_NAME"/>
<gate name="-PEG_RX11+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX11-" symbol="1PIN_NAME"/>
<gate name="-GND@39" symbol="1PIN_NAME"/>
<gate name="-PEG_RX12+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX12-" symbol="1PIN_NAME"/>
<gate name="-GND@40" symbol="1PIN_NAME"/>
<gate name="-PEG_RX13+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX13-" symbol="1PIN_NAME"/>
<gate name="-GND@41" symbol="1PIN_NAME"/>
<gate name="-RSVD@10" symbol="1PIN_NAME"/>
<gate name="-PEG_RX14+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX14-" symbol="1PIN_NAME"/>
<gate name="-GND@42" symbol="1PIN_NAME"/>
<gate name="-PEG_RX15+" symbol="1PIN_NAME"/>
<gate name="-PEG_RX15-" symbol="1PIN_NAME"/>
<gate name="-GND@43" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@21" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@22" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@23" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@24" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@25" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@26" symbol="1PIN_NAME"/>
<gate name="-GND@44" symbol="1PIN_NAME"/>
<gate name="-GND@45" symbol="1PIN_NAME"/>
<gate name="-IDE_D5" symbol="1PIN_NAME"/>
<gate name="-IDE_D10" symbol="1PIN_NAME"/>
<gate name="-IDE_D11" symbol="1PIN_NAME"/>
<gate name="-IDE_D12" symbol="1PIN_NAME"/>
<gate name="-IDE_D4" symbol="1PIN_NAME"/>
<gate name="-IDE_D0" symbol="1PIN_NAME"/>
<gate name="-IDE_REQ" symbol="1PIN_NAME"/>
<gate name="-!IDE_IOW" symbol="1PIN_NAME"/>
<gate name="-!IDE_ACK" symbol="1PIN_NAME"/>
<gate name="-GND@46" symbol="1PIN_NAME"/>
<gate name="-IDE_IRQ" symbol="1PIN_NAME"/>
<gate name="-IDE_A0" symbol="1PIN_NAME"/>
<gate name="-IDE_A1" symbol="1PIN_NAME"/>
<gate name="-IDE_A2" symbol="1PIN_NAME"/>
<gate name="-!IDE_CS1" symbol="1PIN_NAME"/>
<gate name="-!IDE_CS3" symbol="1PIN_NAME"/>
<gate name="-!IDE_RESET" symbol="1PIN_NAME"/>
<gate name="-!PCI_GNT3" symbol="1PIN_NAME"/>
<gate name="-!PCI_REQ3" symbol="1PIN_NAME"/>
<gate name="-GND@47" symbol="1PIN_NAME"/>
<gate name="-PCI_AD1" symbol="1PIN_NAME"/>
<gate name="-PCI_AD3" symbol="1PIN_NAME"/>
<gate name="-PCI_AD5" symbol="1PIN_NAME"/>
<gate name="-PCI_AD7" symbol="1PIN_NAME"/>
<gate name="-PCI_C/!BE0" symbol="1PIN_NAME"/>
<gate name="-PCI_AD9" symbol="1PIN_NAME"/>
<gate name="-PCI_AD11" symbol="1PIN_NAME"/>
<gate name="-PCI_AD13" symbol="1PIN_NAME"/>
<gate name="-PCI_AD15" symbol="1PIN_NAME"/>
<gate name="-GND@48" symbol="1PIN_NAME"/>
<gate name="-PCI_PAR" symbol="1PIN_NAME"/>
<gate name="-!PCI_SERR" symbol="1PIN_NAME"/>
<gate name="-!PCI_STOP" symbol="1PIN_NAME"/>
<gate name="-!PCI_TRDY" symbol="1PIN_NAME"/>
<gate name="-!PCI_FRAME" symbol="1PIN_NAME"/>
<gate name="-PCI_AD16" symbol="1PIN_NAME"/>
<gate name="-PCI_AD18" symbol="1PIN_NAME"/>
<gate name="-PCI_AD20" symbol="1PIN_NAME"/>
<gate name="-PCI_AD22" symbol="1PIN_NAME"/>
<gate name="-GND@49" symbol="1PIN_NAME"/>
<gate name="-PCI_AD24" symbol="1PIN_NAME"/>
<gate name="-PCI_AD26" symbol="1PIN_NAME"/>
<gate name="-PCI_AD28" symbol="1PIN_NAME"/>
<gate name="-PCI_AD30" symbol="1PIN_NAME"/>
<gate name="-!PCI_IRQC" symbol="1PIN_NAME"/>
<gate name="-!PCI_IRQD" symbol="1PIN_NAME"/>
<gate name="-!PCI_CLKRUN" symbol="1PIN_NAME"/>
<gate name="-PCI_M66EN" symbol="1PIN_NAME"/>
<gate name="-PCI_CLK" symbol="1PIN_NAME"/>
<gate name="-GND@50" symbol="1PIN_NAME"/>
<gate name="-PEG_TX0+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX0-" symbol="1PIN_NAME"/>
<gate name="-!PEG_LANE_RV" symbol="1PIN_NAME"/>
<gate name="-PEG_TX1+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX1-" symbol="1PIN_NAME"/>
<gate name="-!TYPE2" symbol="1PIN_NAME"/>
<gate name="-PEG_TX2+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX2-" symbol="1PIN_NAME"/>
<gate name="-GND@51" symbol="1PIN_NAME"/>
<gate name="-PEG_TX3+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX3-" symbol="1PIN_NAME"/>
<gate name="-RSVD@11" symbol="1PIN_NAME"/>
<gate name="-RSVD@12" symbol="1PIN_NAME"/>
<gate name="-PEG_TX4+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX4-" symbol="1PIN_NAME"/>
<gate name="-GND@52" symbol="1PIN_NAME"/>
<gate name="-PEG_TX5+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX5-" symbol="1PIN_NAME"/>
<gate name="-GND@53" symbol="1PIN_NAME"/>
<gate name="-PEG_TX6+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX6-" symbol="1PIN_NAME"/>
<gate name="-SDVO_CLK" symbol="1PIN_NAME"/>
<gate name="-PEG_TX7+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX7-" symbol="1PIN_NAME"/>
<gate name="-GND@54" symbol="1PIN_NAME"/>
<gate name="-IDE_CBLID" symbol="1PIN_NAME"/>
<gate name="-PEG_TX8+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX8-" symbol="1PIN_NAME"/>
<gate name="-GND@55" symbol="1PIN_NAME"/>
<gate name="-PEG_TX9+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX9-" symbol="1PIN_NAME"/>
<gate name="-RSVD@13" symbol="1PIN_NAME"/>
<gate name="-GND@56" symbol="1PIN_NAME"/>
<gate name="-PEG_TX10+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX10-" symbol="1PIN_NAME"/>
<gate name="-GND@57" symbol="1PIN_NAME"/>
<gate name="-PEG_TX11+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX11-" symbol="1PIN_NAME"/>
<gate name="-GND@58" symbol="1PIN_NAME"/>
<gate name="-PEG_TX12+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX12-" symbol="1PIN_NAME"/>
<gate name="-GND@59" symbol="1PIN_NAME"/>
<gate name="-PEG_TX13+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX13-" symbol="1PIN_NAME"/>
<gate name="-GND@60" symbol="1PIN_NAME"/>
<gate name="-!PEG_ENABLE" symbol="1PIN_NAME"/>
<gate name="-PEG_TX14+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX14-" symbol="1PIN_NAME"/>
<gate name="-GND@61" symbol="1PIN_NAME"/>
<gate name="-PEG_TX15+" symbol="1PIN_NAME"/>
<gate name="-PEG_TX15-" symbol="1PIN_NAME"/>
<gate name="-GND@62" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@27" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@28" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@29" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@30" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@31" symbol="1PIN_NAME"/>
<gate name="-VCC_12V@32" symbol="1PIN_NAME"/>
<gate name="-GND@63" symbol="1PIN_NAME"/>
</gates>
<devices>
<device name="" package="C-5353652-36-3">
<connects>
<connect gate="-!AC_RST" pin="1" pad="A30"/>
<connect gate="-!ATA_ACT" pin="1" pad="A28"/>
<connect gate="-!BATLOW" pin="1" pad="A27"/>
<connect gate="-!CB_RESET" pin="1" pad="B50"/>
<connect gate="-!EXCD0_CPPE" pin="1" pad="A49"/>
<connect gate="-!EXCD0_PERST" pin="1" pad="A48"/>
<connect gate="-!EXCD1_CPPE" pin="1" pad="B48"/>
<connect gate="-!EXCD1_PERST" pin="1" pad="B47"/>
<connect gate="-!IDE_ACK" pin="1" pad="D10"/>
<connect gate="-!IDE_CS1" pin="1" pad="D16"/>
<connect gate="-!IDE_CS3" pin="1" pad="D17"/>
<connect gate="-!IDE_IOR" pin="1" pad="C14"/>
<connect gate="-!IDE_IOW" pin="1" pad="D9"/>
<connect gate="-!IDE_RESET" pin="1" pad="D18"/>
<connect gate="-!KBD_RST" pin="1" pad="A86"/>
<connect gate="-!LPC_DRQ0" pin="1" pad="B8"/>
<connect gate="-!PCI_CLKRUN" pin="1" pad="D48"/>
<connect gate="-!PCI_DEVSEL" pin="1" pad="C36"/>
<connect gate="-!PCI_FRAME" pin="1" pad="D36"/>
<connect gate="-!PCI_GNT0" pin="1" pad="C20"/>
<connect gate="-!PCI_GNT1" pin="1" pad="C18"/>
<connect gate="-!PCI_GNT2" pin="1" pad="C16"/>
<connect gate="-!PCI_GNT3" pin="1" pad="D19"/>
<connect gate="-!PCI_IRDY" pin="1" pad="C37"/>
<connect gate="-!PCI_IRQA" pin="1" pad="C49"/>
<connect gate="-!PCI_IRQB" pin="1" pad="C50"/>
<connect gate="-!PCI_IRQC" pin="1" pad="D46"/>
<connect gate="-!PCI_IRQD" pin="1" pad="D47"/>
<connect gate="-!PCI_LOCK" pin="1" pad="C35"/>
<connect gate="-!PCI_PERR" pin="1" pad="C34"/>
<connect gate="-!PCI_PME" pin="1" pad="C15"/>
<connect gate="-!PCI_REQ0" pin="1" pad="C22"/>
<connect gate="-!PCI_REQ1" pin="1" pad="C19"/>
<connect gate="-!PCI_REQ2" pin="1" pad="C17"/>
<connect gate="-!PCI_REQ3" pin="1" pad="D20"/>
<connect gate="-!PCI_RST" pin="1" pad="C23"/>
<connect gate="-!PCI_SERR" pin="1" pad="D33"/>
<connect gate="-!PCI_STOP" pin="1" pad="D34"/>
<connect gate="-!PCI_TRDY" pin="1" pad="D35"/>
<connect gate="-!PEG_ENABLE" pin="1" pad="D97"/>
<connect gate="-!PEG_LANE_RV" pin="1" pad="D54"/>
<connect gate="-!PWRBTN" pin="1" pad="B12"/>
<connect gate="-!SUS_S3" pin="1" pad="A15"/>
<connect gate="-!SUS_S4" pin="1" pad="A18"/>
<connect gate="-!SUS_S5" pin="1" pad="A24"/>
<connect gate="-!SYS_RESET" pin="1" pad="B49"/>
<connect gate="-!THRMTRIP" pin="1" pad="A35"/>
<connect gate="-!TYPE0" pin="1" pad="C54"/>
<connect gate="-!TYPE1" pin="1" pad="C57"/>
<connect gate="-!TYPE2" pin="1" pad="D57"/>
<connect gate="-!USB_0_1_OC" pin="1" pad="B44"/>
<connect gate="-!USB_2_3_OC" pin="1" pad="A44"/>
<connect gate="-!USB_4_5_OC" pin="1" pad="B38"/>
<connect gate="-!USB_6_7_OC" pin="1" pad="A38"/>
<connect gate="-!WAKE0" pin="1" pad="B66"/>
<connect gate="-!WAKE1" pin="1" pad="B67"/>
<connect gate="-AC_BITCLK" pin="1" pad="A32"/>
<connect gate="-AC_SDIN0" pin="1" pad="B30"/>
<connect gate="-AC_SDIN1" pin="1" pad="B29"/>
<connect gate="-AC_SDIN2" pin="1" pad="B28"/>
<connect gate="-AC_SDOUT" pin="1" pad="A33"/>
<connect gate="-AC_SYNC" pin="1" pad="A29"/>
<connect gate="-BIOS_DISABLE" pin="1" pad="A34"/>
<connect gate="-GBE0_!LINK" pin="1" pad="A8"/>
<connect gate="-GBE0_ACT" pin="1" pad="B2"/>
<connect gate="-GBE0_CTREF" pin="1" pad="A14"/>
<connect gate="-GBE0_LINK10" pin="1" pad="A4"/>
<connect gate="-GBE0_LINK10@1" pin="1" pad="A5"/>
<connect gate="-GBE0_MDI0+" pin="1" pad="A13"/>
<connect gate="-GBE0_MDI0-" pin="1" pad="A12"/>
<connect gate="-GBE0_MDI1+" pin="1" pad="A10"/>
<connect gate="-GBE0_MDI1-" pin="1" pad="A9"/>
<connect gate="-GBE0_MDI2+" pin="1" pad="A7"/>
<connect gate="-GBE0_MDI2-" pin="1" pad="A6"/>
<connect gate="-GBE0_MDI3+" pin="1" pad="A3"/>
<connect gate="-GBE0_MDI3-" pin="1" pad="A2"/>
<connect gate="-GND" pin="1" pad="A1"/>
<connect gate="-GND@1" pin="1" pad="A11"/>
<connect gate="-GND@10" pin="1" pad="A80"/>
<connect gate="-GND@11" pin="1" pad="A90"/>
<connect gate="-GND@12" pin="1" pad="A96"/>
<connect gate="-GND@13" pin="1" pad="A100"/>
<connect gate="-GND@14" pin="1" pad="A110"/>
<connect gate="-GND@15" pin="1" pad="B1"/>
<connect gate="-GND@16" pin="1" pad="B11"/>
<connect gate="-GND@17" pin="1" pad="B21"/>
<connect gate="-GND@18" pin="1" pad="B31"/>
<connect gate="-GND@19" pin="1" pad="B41"/>
<connect gate="-GND@2" pin="1" pad="A21"/>
<connect gate="-GND@20" pin="1" pad="B51"/>
<connect gate="-GND@21" pin="1" pad="B60"/>
<connect gate="-GND@22" pin="1" pad="B70"/>
<connect gate="-GND@23" pin="1" pad="B80"/>
<connect gate="-GND@24" pin="1" pad="B90"/>
<connect gate="-GND@25" pin="1" pad="B100"/>
<connect gate="-GND@26" pin="1" pad="B110"/>
<connect gate="-GND@27" pin="1" pad="C1"/>
<connect gate="-GND@28" pin="1" pad="C11"/>
<connect gate="-GND@29" pin="1" pad="C21"/>
<connect gate="-GND@3" pin="1" pad="A31"/>
<connect gate="-GND@30" pin="1" pad="C31"/>
<connect gate="-GND@31" pin="1" pad="C41"/>
<connect gate="-GND@32" pin="1" pad="C51"/>
<connect gate="-GND@33" pin="1" pad="C60"/>
<connect gate="-GND@34" pin="1" pad="C70"/>
<connect gate="-GND@35" pin="1" pad="C76"/>
<connect gate="-GND@36" pin="1" pad="C80"/>
<connect gate="-GND@37" pin="1" pad="C84"/>
<connect gate="-GND@38" pin="1" pad="C87"/>
<connect gate="-GND@39" pin="1" pad="C90"/>
<connect gate="-GND@4" pin="1" pad="A41"/>
<connect gate="-GND@40" pin="1" pad="C93"/>
<connect gate="-GND@41" pin="1" pad="C96"/>
<connect gate="-GND@42" pin="1" pad="C100"/>
<connect gate="-GND@43" pin="1" pad="C103"/>
<connect gate="-GND@44" pin="1" pad="C110"/>
<connect gate="-GND@45" pin="1" pad="D1"/>
<connect gate="-GND@46" pin="1" pad="D11"/>
<connect gate="-GND@47" pin="1" pad="D21"/>
<connect gate="-GND@48" pin="1" pad="D31"/>
<connect gate="-GND@49" pin="1" pad="D41"/>
<connect gate="-GND@5" pin="1" pad="A51"/>
<connect gate="-GND@50" pin="1" pad="D51"/>
<connect gate="-GND@51" pin="1" pad="D60"/>
<connect gate="-GND@52" pin="1" pad="D67"/>
<connect gate="-GND@53" pin="1" pad="D70"/>
<connect gate="-GND@54" pin="1" pad="D76"/>
<connect gate="-GND@55" pin="1" pad="D80"/>
<connect gate="-GND@56" pin="1" pad="D84"/>
<connect gate="-GND@57" pin="1" pad="D87"/>
<connect gate="-GND@58" pin="1" pad="D90"/>
<connect gate="-GND@59" pin="1" pad="D93"/>
<connect gate="-GND@6" pin="1" pad="A57"/>
<connect gate="-GND@60" pin="1" pad="D96"/>
<connect gate="-GND@61" pin="1" pad="D100"/>
<connect gate="-GND@62" pin="1" pad="D103"/>
<connect gate="-GND@63" pin="1" pad="D110"/>
<connect gate="-GND@7" pin="1" pad="A60"/>
<connect gate="-GND@8" pin="1" pad="A66"/>
<connect gate="-GND@9" pin="1" pad="A70"/>
<connect gate="-GPI0" pin="1" pad="A54"/>
<connect gate="-GPI1" pin="1" pad="A63"/>
<connect gate="-GPI2" pin="1" pad="A67"/>
<connect gate="-GPI3" pin="1" pad="A85"/>
<connect gate="-GPO0" pin="1" pad="A93"/>
<connect gate="-GPO1" pin="1" pad="B54"/>
<connect gate="-GPO2" pin="1" pad="B57"/>
<connect gate="-GPO3" pin="1" pad="B63"/>
<connect gate="-I2C_CK" pin="1" pad="B33"/>
<connect gate="-I2C_DAT" pin="1" pad="B34"/>
<connect gate="-IDE_A0" pin="1" pad="D13"/>
<connect gate="-IDE_A1" pin="1" pad="D14"/>
<connect gate="-IDE_A2" pin="1" pad="D15"/>
<connect gate="-IDE_CBLID" pin="1" pad="D77"/>
<connect gate="-IDE_D0" pin="1" pad="D7"/>
<connect gate="-IDE_D1" pin="1" pad="C10"/>
<connect gate="-IDE_D10" pin="1" pad="D3"/>
<connect gate="-IDE_D11" pin="1" pad="D4"/>
<connect gate="-IDE_D12" pin="1" pad="D5"/>
<connect gate="-IDE_D13" pin="1" pad="C9"/>
<connect gate="-IDE_D14" pin="1" pad="C12"/>
<connect gate="-IDE_D15" pin="1" pad="C5"/>
<connect gate="-IDE_D2" pin="1" pad="C8"/>
<connect gate="-IDE_D3" pin="1" pad="C4"/>
<connect gate="-IDE_D4" pin="1" pad="D6"/>
<connect gate="-IDE_D5" pin="1" pad="D2"/>
<connect gate="-IDE_D6" pin="1" pad="C3"/>
<connect gate="-IDE_D7" pin="1" pad="C2"/>
<connect gate="-IDE_D8" pin="1" pad="C6"/>
<connect gate="-IDE_D9" pin="1" pad="C7"/>
<connect gate="-IDE_IORDY" pin="1" pad="C13"/>
<connect gate="-IDE_IRQ" pin="1" pad="D12"/>
<connect gate="-IDE_REQ" pin="1" pad="D8"/>
<connect gate="-KBD_A20GATE" pin="1" pad="A87"/>
<connect gate="-LPC_AD0" pin="1" pad="B4"/>
<connect gate="-LPC_AD1" pin="1" pad="B5"/>
<connect gate="-LPC_AD2" pin="1" pad="B6"/>
<connect gate="-LPC_AD3" pin="1" pad="B7"/>
<connect gate="-LPC_CLK" pin="1" pad="B10"/>
<connect gate="-LPC_DRQ1!" pin="1" pad="B9"/>
<connect gate="-LPC_FRAME!" pin="1" pad="B3"/>
<connect gate="-LPC_SERIRQ" pin="1" pad="A50"/>
<connect gate="-LVDS_A0+" pin="1" pad="A71"/>
<connect gate="-LVDS_A0-" pin="1" pad="A72"/>
<connect gate="-LVDS_A1+" pin="1" pad="A73"/>
<connect gate="-LVDS_A1-" pin="1" pad="A74"/>
<connect gate="-LVDS_A2+" pin="1" pad="A75"/>
<connect gate="-LVDS_A2-" pin="1" pad="A76"/>
<connect gate="-LVDS_A3+" pin="1" pad="A78"/>
<connect gate="-LVDS_A3-" pin="1" pad="A79"/>
<connect gate="-LVDS_A_CK+" pin="1" pad="A81"/>
<connect gate="-LVDS_A_CK-" pin="1" pad="A82"/>
<connect gate="-LVDS_B0+" pin="1" pad="B71"/>
<connect gate="-LVDS_B0-" pin="1" pad="B72"/>
<connect gate="-LVDS_B1+" pin="1" pad="B73"/>
<connect gate="-LVDS_B1-" pin="1" pad="B74"/>
<connect gate="-LVDS_B2+" pin="1" pad="B75"/>
<connect gate="-LVDS_B2-" pin="1" pad="B76"/>
<connect gate="-LVDS_B3+" pin="1" pad="B77"/>
<connect gate="-LVDS_B3-" pin="1" pad="B78"/>
<connect gate="-LVDS_BKLT_CTRL" pin="1" pad="B83"/>
<connect gate="-LVDS_BKLT_EN" pin="1" pad="B79"/>
<connect gate="-LVDS_B_CK+" pin="1" pad="B81"/>
<connect gate="-LVDS_B_CK-" pin="1" pad="B82"/>
<connect gate="-LVDS_I2C_CK" pin="1" pad="A83"/>
<connect gate="-LVDS_I2C_DAT" pin="1" pad="A84"/>
<connect gate="-LVDS_VDD_EN" pin="1" pad="A77"/>
<connect gate="-PCIE0_CK_REF+" pin="1" pad="A88"/>
<connect gate="-PCIE0_CK_REF-" pin="1" pad="A89"/>
<connect gate="-PCIE_RX0+" pin="1" pad="B68"/>
<connect gate="-PCIE_RX0-" pin="1" pad="B69"/>
<connect gate="-PCIE_RX1+" pin="1" pad="B64"/>
<connect gate="-PCIE_RX1-" pin="1" pad="B65"/>
<connect gate="-PCIE_RX2+" pin="1" pad="B61"/>
<connect gate="-PCIE_RX2-" pin="1" pad="B62"/>
<connect gate="-PCIE_RX3+" pin="1" pad="B58"/>
<connect gate="-PCIE_RX3-" pin="1" pad="B59"/>
<connect gate="-PCIE_RX4+" pin="1" pad="B55"/>
<connect gate="-PCIE_RX4-" pin="1" pad="B56"/>
<connect gate="-PCIE_RX5+" pin="1" pad="B52"/>
<connect gate="-PCIE_RX5-" pin="1" pad="B53"/>
<connect gate="-PCIE_TX0+" pin="1" pad="A68"/>
<connect gate="-PCIE_TX0-" pin="1" pad="A69"/>
<connect gate="-PCIE_TX1+" pin="1" pad="A64"/>
<connect gate="-PCIE_TX1-" pin="1" pad="A65"/>
<connect gate="-PCIE_TX2+" pin="1" pad="A61"/>
<connect gate="-PCIE_TX2-" pin="1" pad="A62"/>
<connect gate="-PCIE_TX3+" pin="1" pad="A58"/>
<connect gate="-PCIE_TX3-" pin="1" pad="A59"/>
<connect gate="-PCIE_TX4+" pin="1" pad="A55"/>
<connect gate="-PCIE_TX4-" pin="1" pad="A56"/>
<connect gate="-PCIE_TX5+" pin="1" pad="A52"/>
<connect gate="-PCIE_TX5-" pin="1" pad="A53"/>
<connect gate="-PCI_AD0" pin="1" pad="C24"/>
<connect gate="-PCI_AD1" pin="1" pad="D22"/>
<connect gate="-PCI_AD10" pin="1" pad="C29"/>
<connect gate="-PCI_AD11" pin="1" pad="D28"/>
<connect gate="-PCI_AD12" pin="1" pad="C30"/>
<connect gate="-PCI_AD13" pin="1" pad="D29"/>
<connect gate="-PCI_AD14" pin="1" pad="C32"/>
<connect gate="-PCI_AD15" pin="1" pad="D30"/>
<connect gate="-PCI_AD16" pin="1" pad="D37"/>
<connect gate="-PCI_AD17" pin="1" pad="C39"/>
<connect gate="-PCI_AD18" pin="1" pad="D38"/>
<connect gate="-PCI_AD19" pin="1" pad="C40"/>
<connect gate="-PCI_AD2" pin="1" pad="C25"/>
<connect gate="-PCI_AD20" pin="1" pad="D39"/>
<connect gate="-PCI_AD21" pin="1" pad="C42"/>
<connect gate="-PCI_AD22" pin="1" pad="D40"/>
<connect gate="-PCI_AD23" pin="1" pad="C43"/>
<connect gate="-PCI_AD24" pin="1" pad="D42"/>
<connect gate="-PCI_AD25" pin="1" pad="C45"/>
<connect gate="-PCI_AD26" pin="1" pad="D43"/>
<connect gate="-PCI_AD27" pin="1" pad="C46"/>
<connect gate="-PCI_AD28" pin="1" pad="D44"/>
<connect gate="-PCI_AD29" pin="1" pad="C47"/>
<connect gate="-PCI_AD3" pin="1" pad="D23"/>
<connect gate="-PCI_AD30" pin="1" pad="D45"/>
<connect gate="-PCI_AD31" pin="1" pad="C48"/>
<connect gate="-PCI_AD4" pin="1" pad="C26"/>
<connect gate="-PCI_AD5" pin="1" pad="D24"/>
<connect gate="-PCI_AD6" pin="1" pad="C27"/>
<connect gate="-PCI_AD7" pin="1" pad="D25"/>
<connect gate="-PCI_AD8" pin="1" pad="C28"/>
<connect gate="-PCI_AD9" pin="1" pad="D27"/>
<connect gate="-PCI_C/!BE0" pin="1" pad="D26"/>
<connect gate="-PCI_C/!BE1" pin="1" pad="C33"/>
<connect gate="-PCI_C/!BE2" pin="1" pad="C38"/>
<connect gate="-PCI_C/!BE3" pin="1" pad="C44"/>
<connect gate="-PCI_CLK" pin="1" pad="D50"/>
<connect gate="-PCI_M66EN" pin="1" pad="D49"/>
<connect gate="-PCI_PAR" pin="1" pad="D32"/>
<connect gate="-PEG_RX0+" pin="1" pad="C52"/>
<connect gate="-PEG_RX0-" pin="1" pad="C53"/>
<connect gate="-PEG_RX1+" pin="1" pad="C55"/>
<connect gate="-PEG_RX1-" pin="1" pad="C56"/>
<connect gate="-PEG_RX10+" pin="1" pad="C85"/>
<connect gate="-PEG_RX10-" pin="1" pad="C86"/>
<connect gate="-PEG_RX11+" pin="1" pad="C88"/>
<connect gate="-PEG_RX11-" pin="1" pad="C89"/>
<connect gate="-PEG_RX12+" pin="1" pad="C91"/>
<connect gate="-PEG_RX12-" pin="1" pad="C92"/>
<connect gate="-PEG_RX13+" pin="1" pad="C94"/>
<connect gate="-PEG_RX13-" pin="1" pad="C95"/>
<connect gate="-PEG_RX14+" pin="1" pad="C98"/>
<connect gate="-PEG_RX14-" pin="1" pad="C99"/>
<connect gate="-PEG_RX15+" pin="1" pad="C101"/>
<connect gate="-PEG_RX15-" pin="1" pad="C102"/>
<connect gate="-PEG_RX2+" pin="1" pad="C58"/>
<connect gate="-PEG_RX2-" pin="1" pad="C59"/>
<connect gate="-PEG_RX3+" pin="1" pad="C61"/>
<connect gate="-PEG_RX3-" pin="1" pad="C62"/>
<connect gate="-PEG_RX4+" pin="1" pad="C65"/>
<connect gate="-PEG_RX4-" pin="1" pad="C66"/>
<connect gate="-PEG_RX5+" pin="1" pad="C68"/>
<connect gate="-PEG_RX5-" pin="1" pad="C69"/>
<connect gate="-PEG_RX6+" pin="1" pad="C71"/>
<connect gate="-PEG_RX6-" pin="1" pad="C72"/>
<connect gate="-PEG_RX7+" pin="1" pad="C74"/>
<connect gate="-PEG_RX7-" pin="1" pad="C75"/>
<connect gate="-PEG_RX8+" pin="1" pad="C78"/>
<connect gate="-PEG_RX8-" pin="1" pad="C79"/>
<connect gate="-PEG_RX9+" pin="1" pad="C81"/>
<connect gate="-PEG_RX9-" pin="1" pad="C82"/>
<connect gate="-PEG_TX0+" pin="1" pad="D52"/>
<connect gate="-PEG_TX0-" pin="1" pad="D53"/>
<connect gate="-PEG_TX1+" pin="1" pad="D55"/>
<connect gate="-PEG_TX1-" pin="1" pad="D56"/>
<connect gate="-PEG_TX10+" pin="1" pad="D85"/>
<connect gate="-PEG_TX10-" pin="1" pad="D86"/>
<connect gate="-PEG_TX11+" pin="1" pad="D88"/>
<connect gate="-PEG_TX11-" pin="1" pad="D89"/>
<connect gate="-PEG_TX12+" pin="1" pad="D91"/>
<connect gate="-PEG_TX12-" pin="1" pad="D92"/>
<connect gate="-PEG_TX13+" pin="1" pad="D94"/>
<connect gate="-PEG_TX13-" pin="1" pad="D95"/>
<connect gate="-PEG_TX14+" pin="1" pad="D98"/>
<connect gate="-PEG_TX14-" pin="1" pad="D99"/>
<connect gate="-PEG_TX15+" pin="1" pad="D101"/>
<connect gate="-PEG_TX15-" pin="1" pad="D102"/>
<connect gate="-PEG_TX2+" pin="1" pad="D58"/>
<connect gate="-PEG_TX2-" pin="1" pad="D59"/>
<connect gate="-PEG_TX3+" pin="1" pad="D61"/>
<connect gate="-PEG_TX3-" pin="1" pad="D62"/>
<connect gate="-PEG_TX4+" pin="1" pad="D65"/>
<connect gate="-PEG_TX4-" pin="1" pad="D66"/>
<connect gate="-PEG_TX5+" pin="1" pad="D68"/>
<connect gate="-PEG_TX5-" pin="1" pad="D69"/>
<connect gate="-PEG_TX6+" pin="1" pad="D71"/>
<connect gate="-PEG_TX6-" pin="1" pad="D72"/>
<connect gate="-PEG_TX7+" pin="1" pad="D74"/>
<connect gate="-PEG_TX7-" pin="1" pad="D75"/>
<connect gate="-PEG_TX8+" pin="1" pad="D78"/>
<connect gate="-PEG_TX8-" pin="1" pad="D79"/>
<connect gate="-PEG_TX9+" pin="1" pad="D81"/>
<connect gate="-PEG_TX9-" pin="1" pad="D82"/>
<connect gate="-PWR_OK" pin="1" pad="B24"/>
<connect gate="-RSVD" pin="1" pad="A91"/>
<connect gate="-RSVD@1" pin="1" pad="A92"/>
<connect gate="-RSVD@10" pin="1" pad="C97"/>
<connect gate="-RSVD@11" pin="1" pad="D63"/>
<connect gate="-RSVD@12" pin="1" pad="D64"/>
<connect gate="-RSVD@13" pin="1" pad="D83"/>
<connect gate="-RSVD@2" pin="1" pad="A94"/>
<connect gate="-RSVD@3" pin="1" pad="A95"/>
<connect gate="-RSVD@4" pin="1" pad="B88"/>
<connect gate="-RSVD@5" pin="1" pad="C63"/>
<connect gate="-RSVD@6" pin="1" pad="C64"/>
<connect gate="-RSVD@7" pin="1" pad="C67"/>
<connect gate="-RSVD@8" pin="1" pad="C77"/>
<connect gate="-RSVD@9" pin="1" pad="C83"/>
<connect gate="-SATA0_RX+" pin="1" pad="A19"/>
<connect gate="-SATA0_RX-" pin="1" pad="A20"/>
<connect gate="-SATA0_TX+" pin="1" pad="A16"/>
<connect gate="-SATA0_TX-" pin="1" pad="A17"/>
<connect gate="-SATA1_RX+" pin="1" pad="B19"/>
<connect gate="-SATA1_RX-" pin="1" pad="B20"/>
<connect gate="-SATA1_TX+" pin="1" pad="B16"/>
<connect gate="-SATA1_TX-" pin="1" pad="B17"/>
<connect gate="-SATA2_RX+" pin="1" pad="A25"/>
<connect gate="-SATA2_RX-" pin="1" pad="A26"/>
<connect gate="-SATA2_TX+" pin="1" pad="A22"/>
<connect gate="-SATA2_TX-" pin="1" pad="A23"/>
<connect gate="-SATA3_RX+" pin="1" pad="B25"/>
<connect gate="-SATA3_RX-" pin="1" pad="B26"/>
<connect gate="-SATA3_TX+" pin="1" pad="B22"/>
<connect gate="-SATA3_TX-" pin="1" pad="B23"/>
<connect gate="-SDVO_CLK" pin="1" pad="D73"/>
<connect gate="-SDVO_DATA" pin="1" pad="C73"/>
<connect gate="-SMB_ALERT!" pin="1" pad="B15"/>
<connect gate="-SMB_CK" pin="1" pad="B13"/>
<connect gate="-SMB_DAT" pin="1" pad="B14"/>
<connect gate="-SPKR" pin="1" pad="B32"/>
<connect gate="-SUS_STAT!" pin="1" pad="B18"/>
<connect gate="-THRM!" pin="1" pad="B35"/>
<connect gate="-TV_DAC_A" pin="1" pad="B97"/>
<connect gate="-TV_DAC_B" pin="1" pad="B98"/>
<connect gate="-TV_DAC_C" pin="1" pad="B99"/>
<connect gate="-USB0+" pin="1" pad="A46"/>
<connect gate="-USB0-" pin="1" pad="A45"/>
<connect gate="-USB1+" pin="1" pad="B46"/>
<connect gate="-USB1-" pin="1" pad="B45"/>
<connect gate="-USB2+" pin="1" pad="A43"/>
<connect gate="-USB2-" pin="1" pad="A42"/>
<connect gate="-USB3+" pin="1" pad="B43"/>
<connect gate="-USB3-" pin="1" pad="B42"/>
<connect gate="-USB4+" pin="1" pad="A40"/>
<connect gate="-USB4-" pin="1" pad="A39"/>
<connect gate="-USB5+" pin="1" pad="B40"/>
<connect gate="-USB5-" pin="1" pad="B39"/>
<connect gate="-USB6+" pin="1" pad="A37"/>
<connect gate="-USB6-" pin="1" pad="A36"/>
<connect gate="-USB7+" pin="1" pad="B37"/>
<connect gate="-USB7-" pin="1" pad="B36"/>
<connect gate="-VCC_12V" pin="1" pad="A97"/>
<connect gate="-VCC_12V@1" pin="1" pad="A98"/>
<connect gate="-VCC_12V@10" pin="1" pad="A108"/>
<connect gate="-VCC_12V@11" pin="1" pad="A109"/>
<connect gate="-VCC_12V@12" pin="1" pad="B101"/>
<connect gate="-VCC_12V@13" pin="1" pad="B102"/>
<connect gate="-VCC_12V@14" pin="1" pad="B103"/>
<connect gate="-VCC_12V@15" pin="1" pad="B104"/>
<connect gate="-VCC_12V@16" pin="1" pad="B105"/>
<connect gate="-VCC_12V@17" pin="1" pad="B106"/>
<connect gate="-VCC_12V@18" pin="1" pad="B107"/>
<connect gate="-VCC_12V@19" pin="1" pad="B108"/>
<connect gate="-VCC_12V@2" pin="1" pad="A99"/>
<connect gate="-VCC_12V@20" pin="1" pad="B109"/>
<connect gate="-VCC_12V@21" pin="1" pad="C104"/>
<connect gate="-VCC_12V@22" pin="1" pad="C105"/>
<connect gate="-VCC_12V@23" pin="1" pad="C106"/>
<connect gate="-VCC_12V@24" pin="1" pad="C107"/>
<connect gate="-VCC_12V@25" pin="1" pad="C108"/>
<connect gate="-VCC_12V@26" pin="1" pad="C109"/>
<connect gate="-VCC_12V@27" pin="1" pad="D104"/>
<connect gate="-VCC_12V@28" pin="1" pad="D105"/>
<connect gate="-VCC_12V@29" pin="1" pad="D106"/>
<connect gate="-VCC_12V@3" pin="1" pad="A101"/>
<connect gate="-VCC_12V@30" pin="1" pad="D107"/>
<connect gate="-VCC_12V@31" pin="1" pad="D108"/>
<connect gate="-VCC_12V@32" pin="1" pad="D109"/>
<connect gate="-VCC_12V@4" pin="1" pad="A102"/>
<connect gate="-VCC_12V@5" pin="1" pad="A103"/>
<connect gate="-VCC_12V@6" pin="1" pad="A104"/>
<connect gate="-VCC_12V@7" pin="1" pad="A105"/>
<connect gate="-VCC_12V@8" pin="1" pad="A106"/>
<connect gate="-VCC_12V@9" pin="1" pad="A107"/>
<connect gate="-VCC_5V_SBY" pin="1" pad="B84"/>
<connect gate="-VCC_5V_SBY@1" pin="1" pad="B85"/>
<connect gate="-VCC_5V_SBY@2" pin="1" pad="B86"/>
<connect gate="-VCC_5V_SBY@3" pin="1" pad="B87"/>
<connect gate="-VCC_RTC" pin="1" pad="A47"/>
<connect gate="-VGA_BLU" pin="1" pad="B92"/>
<connect gate="-VGA_GRN" pin="1" pad="B91"/>
<connect gate="-VGA_HSYNC" pin="1" pad="B93"/>
<connect gate="-VGA_I2C_CK" pin="1" pad="B95"/>
<connect gate="-VGA_I2C_DAT" pin="1" pad="B96"/>
<connect gate="-VGA_RED" pin="1" pad="B89"/>
<connect gate="-VGA_VSYNC" pin="1" pad="B94"/>
<connect gate="-WDT" pin="1" pad="B27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
