<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Freescale&lt;/b&gt;&lt;p&gt;
www.freescale.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="QFP-12X12-80E">
<description>&lt;b&gt;QFP80&lt;/b&gt;&lt;p&gt;
quad flat pack, square</description>
</package>
<package name="TQFP48_7X7">
<description>&lt;b&gt;48-Pin LQFP (Case #932)&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC68HC908AP64.pdf</description>
</package>
<package name="QFP44">
<description>&lt;b&gt;44-Pin QFP (Case #824A)&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC68HC908AP64.pdf</description>
</package>
<package name="PSDIP_42">
<description>&lt;b&gt;42-Pin Shrink Dual In-Line Package (SDIP)&lt;/b&gt; Case #858&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC68HC908AP64.pdf</description>
</package>
<package name="QFP160">
<description>&lt;b&gt;QFP160&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 22&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="MAPGBA196">
</package>
<package name="SQFP-S-20X20-144">
<description>&lt;b&gt;QFP144&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="SQFP-S-20X20-112">
<description>&lt;b&gt;LQFP112 20x20mm&lt;/b&gt;&lt;p&gt;
112-Pin LQFP Mechanical Dimensions (Case No. 987)&lt;br&gt;
Source: www.freescale.com .. MC9S12XF512V1RM.pdf</description>
</package>
<package name="SQFP-S-10X10-64">
<description>&lt;b&gt;QFP64&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="HSOP44">
<description>&lt;b&gt;44 LEAD HSOP W/PROTRUDING HEADSINK&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/shared/doc/package_info/98ARH98330A.pdf</description>
</package>
<package name="QFN48">
<description>&lt;b&gt;48-pin QFN 7 x 7 mm LF48&lt;/b&gt;&lt;p&gt;
48 Quad Flat Package No Leads&lt;br&gt;
Source: http://v4.cypress.com/cfuploads/img/products/cywusb6934.pdf</description>
</package>
<package name="QFN32">
<description>&lt;b&gt;QFN 32&lt;/b&gt; 5 x 5 mm&lt;p&gt;
Source: http://datasheets.maxim-ic.com/en/ds/MAX7042.pdf</description>
</package>
</packages>
<symbols>
<symbol name="FSA95601">
<pin name="PWMCH1BLO" direction="out"/>
<pin name="VSSIOCH1" direction="in"/>
<pin name="PWMCH1ALO" direction="out"/>
<pin name="PWMCH1AHI" direction="out"/>
<pin name="VDDIOCH01" direction="in"/>
<pin name="PWMCH0BHI" direction="out"/>
<pin name="PWMCH0BLO" direction="out"/>
<pin name="VSSIOCH0" direction="in"/>
<pin name="PWMCH0ALO" direction="out"/>
<pin name="PWMCH0AHI" direction="out"/>
<pin name="VDDD" direction="in"/>
<pin name="VSSD" direction="in"/>
<pin name="CAPDIGP" direction="out"/>
<pin name="IRQB" direction="out"/>
<pin name="SDIN0" direction="in"/>
<pin name="SDIN1" direction="in"/>
<pin name="SDIN2"/>
<pin name="SCLK" direction="in"/>
<pin name="LRCLK" direction="in"/>
<pin name="MOSI_A0" direction="in"/>
<pin name="MISO_SDA"/>
<pin name="VDDDIO" direction="in"/>
<pin name="VSSDIO" direction="in"/>
<pin name="SCK_SCL" direction="in"/>
<pin name="CSB_A1" direction="in"/>
<pin name="I2C_SPIB_MUTEB" direction="in"/>
<pin name="RESETB" direction="in"/>
<pin name="PWRDNB" direction="in"/>
<pin name="TESTEN" direction="in"/>
<pin name="VDDADC" direction="in"/>
<pin name="CLKOUTP" direction="out"/>
<pin name="CLKOUTM" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="XTALGND" direction="in"/>
<pin name="VDDOSC" direction="in"/>
<pin name="CAPVCOP" direction="out"/>
<pin name="CAPVCOM" direction="in"/>
<pin name="VDDA2" direction="in"/>
<pin name="VDDCLK" direction="in"/>
<pin name="VREF" direction="out"/>
<pin name="PWMREF" direction="in"/>
<pin name="VDDINT" direction="in"/>
<pin name="FDBKCH5B" direction="in"/>
<pin name="FDBKCH5A" direction="in"/>
<pin name="VSSSH7" direction="in"/>
<pin name="FDBKCH4B" direction="in"/>
<pin name="FDBKCH4A" direction="in"/>
<pin name="FDBKCH3B" direction="in"/>
<pin name="FDBKCH3A" direction="in"/>
<pin name="FDBKCH2B" direction="in"/>
<pin name="FDBKCH2A" direction="in"/>
<pin name="FDBKCH1B" direction="in"/>
<pin name="FDBKCH1A" direction="in"/>
<pin name="VSSSH2" direction="in"/>
<pin name="FDBKCH0B" direction="in"/>
<pin name="FDBKCH0A" direction="in"/>
<pin name="PWMCH5BHI" direction="out"/>
<pin name="PWMCH5BLO" direction="out"/>
<pin name="VSSIOCH5" direction="in"/>
<pin name="PWMCH5ALO" direction="out"/>
<pin name="PWMCH5AHI" direction="out"/>
<pin name="VDDIOCH45" direction="in"/>
<pin name="PWMCH4BHI" direction="out"/>
<pin name="PWMCH4BLO" direction="out"/>
<pin name="VSSIOCH4" direction="in"/>
<pin name="PWMCH4ALO" direction="out"/>
<pin name="PWMCH4AHI" direction="out"/>
<pin name="PWMCH3BHI" direction="out"/>
<pin name="PWMCH3BLO" direction="out"/>
<pin name="VSSIOCH3" direction="in"/>
<pin name="PWMCH3ALO" direction="out"/>
<pin name="PWMCH3AHI" direction="out"/>
<pin name="VDDIOCH23" direction="in"/>
<pin name="PWMCH2BHI" direction="out"/>
<pin name="PWMCH2BLO" direction="out"/>
<pin name="VSSIOCH2" direction="in"/>
<pin name="PWMCH2ALO" direction="out"/>
<pin name="PWMCH2AHI" direction="out"/>
<pin name="PWMCH1BHI" direction="out"/>
<pin name="VSS_EXP" direction="in"/>
</symbol>
<symbol name="68HC908AP8_V2">
<pin name="PTD2/KBI2"/>
<pin name="PTD1/KBI1"/>
<pin name="PTB7/T2CH1"/>
<pin name="PTD0/KBI0"/>
<pin name="CGMXFC" direction="in"/>
<pin name="PTB6/T2CH0"/>
<pin name="VREG" direction="out"/>
<pin name="PTB5/T1CH1"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="PTB4/T1CH0"/>
<pin name="!IRQ1" direction="in"/>
<pin name="PTB3/RXD"/>
<pin name="!RST" direction="in"/>
<pin name="PTB2/TXD"/>
<pin name="PTB1/SCL"/>
<pin name="PTB0/SDA"/>
<pin name="PTC7/SCRXD"/>
<pin name="PTC6/SCTXD"/>
<pin name="PTC5/SPSCK"/>
<pin name="PTC4/!SS"/>
<pin name="PTC3/MOSI"/>
<pin name="PTC2/MISO"/>
<pin name="PTA7/ADC7"/>
<pin name="PTA6/ADC6"/>
<pin name="PTA5/ADC5"/>
<pin name="PTA4/ADC4"/>
<pin name="PTA3/ADC3"/>
<pin name="PTA2/ADC2"/>
<pin name="PTA1/ADC1"/>
<pin name="PTA0/ADC0"/>
<pin name="VREFL" direction="pas"/>
<pin name="VREFH" direction="pas"/>
<pin name="PTD7/KBI7"/>
<pin name="PTD6/KBI6"/>
<pin name="PTD5/KBI5"/>
<pin name="PTD4/KBI4"/>
<pin name="PTD3/KBI3"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="PTC1"/>
<pin name="PTC0/!IRQ2"/>
</symbol>
<symbol name="68HC908AP8_V1">
<pin name="PTD2/KBI2"/>
<pin name="PTD1/KBI1"/>
<pin name="PTB7/T2CH1"/>
<pin name="PTD0/KBI0"/>
<pin name="CGMXFC" direction="in"/>
<pin name="PTB6/T2CH0"/>
<pin name="VREG" direction="out"/>
<pin name="PTB5/T2CH1"/>
<pin name="VDD" direction="pwr"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="PTB4/T1CH0"/>
<pin name="!IRQ1" direction="in"/>
<pin name="PRB3/RXD"/>
<pin name="!RST" direction="in"/>
<pin name="PTB2/TXD"/>
<pin name="PTB1/SCL"/>
<pin name="PTB0/SDA"/>
<pin name="PTC7/SCRXD"/>
<pin name="PTC6/SCTXD"/>
<pin name="PTC5/SPSCK"/>
<pin name="PTC4/!SS"/>
<pin name="PTC3/MOSI"/>
<pin name="PTC2/MISO"/>
<pin name="PTA7/ADC7"/>
<pin name="PTA6/ADC6"/>
<pin name="PTA5/ADC5"/>
<pin name="PTA4/ADC4"/>
<pin name="PTA3/ADC3"/>
<pin name="PTA2/ADC2"/>
<pin name="PTA1/ADC1"/>
<pin name="PTA0/ADC0"/>
<pin name="VREFL" direction="pas"/>
<pin name="VREFH" direction="pas"/>
<pin name="PTD7/KBI7"/>
<pin name="PTD6/KBI6"/>
<pin name="PTD5/KBI5"/>
<pin name="PTD4/KBI4"/>
<pin name="PTD3/KBI3"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
</symbol>
<symbol name="MCF5372CAB180">
<pin name="FEC_TXD1" direction="out"/>
<pin name="FEC_TXD0" direction="out"/>
<pin name="FEC_MDIO"/>
<pin name="FEC_MDC" direction="out"/>
<pin name="DT0IN" direction="in"/>
<pin name="DT1IN" direction="in"/>
<pin name="DT2IN" direction="in"/>
<pin name="DT3IN" direction="in"/>
<pin name="EVDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="SD_VDD@1" direction="pwr"/>
<pin name="!TS" direction="out"/>
<pin name="!SD_WE" direction="out"/>
<pin name="SD_CKE" direction="out"/>
<pin name="!SD_CS0" direction="out"/>
<pin name="D15"/>
<pin name="D14"/>
<pin name="D13"/>
<pin name="D12"/>
<pin name="D11"/>
<pin name="D10"/>
<pin name="D9"/>
<pin name="D8"/>
<pin name="!BE/BWE1" direction="out"/>
<pin name="SD_DQS1/3" direction="out"/>
<pin name="!BE/BWE3" direction="out"/>
<pin name="D31"/>
<pin name="D30"/>
<pin name="D29"/>
<pin name="D28"/>
<pin name="D27"/>
<pin name="D26"/>
<pin name="D25"/>
<pin name="D24"/>
<pin name="SD_SDR_DQS" direction="out"/>
<pin name="IVDD@1" direction="pwr"/>
<pin name="SD_CLK" direction="out"/>
<pin name="!SD_CLK" direction="out"/>
<pin name="SD_VDD@2" direction="pwr"/>
<pin name="FB_CLK" direction="out"/>
<pin name="SD_VDD@3" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="SD_A10" direction="out"/>
<pin name="!SD_SCAS" direction="out"/>
<pin name="!SD_SRAS" direction="out"/>
<pin name="D23"/>
<pin name="D22"/>
<pin name="D21"/>
<pin name="D20"/>
<pin name="D19"/>
<pin name="D18"/>
<pin name="D17"/>
<pin name="D16"/>
<pin name="!BE/BWE2" direction="out"/>
<pin name="SD_DQS2" direction="out"/>
<pin name="!BE/BWE0" direction="out"/>
<pin name="D7"/>
<pin name="D6"/>
<pin name="D5"/>
<pin name="D4"/>
<pin name="D3"/>
<pin name="D2"/>
<pin name="D1"/>
<pin name="D0"/>
<pin name="R/!W" direction="out"/>
<pin name="!OE" direction="out"/>
<pin name="SD_VDD@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="EVDD@2" direction="pwr"/>
<pin name="PSTCLK" direction="out"/>
<pin name="EVDD@3" direction="pwr"/>
<pin name="!RCON" direction="in"/>
<pin name="ALLPST" direction="out"/>
<pin name="DSO" direction="out"/>
<pin name="QSPI_DIN" direction="in"/>
<pin name="QSPI_DOUT" direction="out"/>
<pin name="QSPI_CLK" direction="out"/>
<pin name="QSPI_CS2" direction="out"/>
<pin name="IVDD@2" direction="pwr"/>
<pin name="U0RXD" direction="in"/>
<pin name="EVDD@4" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="U0TXD" direction="out"/>
<pin name="!U0RTS" direction="out"/>
<pin name="!U0CTS" direction="in"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="TMS/!BKPT" direction="in"/>
<pin name="!TRST!/DSCLK" direction="in"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="DSI" direction="in"/>
<pin name="EXTAL" direction="in"/>
<pin name="DRAMSEL" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="EVDD@5" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="JTAG_EN" direction="in"/>
<pin name="IVDD@3" direction="pwr"/>
<pin name="PLL_VSS" direction="pwr"/>
<pin name="PLL_VDD" direction="pwr"/>
<pin name="!IRQ1" direction="in"/>
<pin name="!IRQ4" direction="in"/>
<pin name="!IRQ7" direction="in"/>
<pin name="EVDD@6" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="SD_VDD@5" direction="pwr"/>
<pin name="!TA" direction="in"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="SD_VDD@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="A14" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="IVDD@4" direction="pwr"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="!VB_CS4!/A22" direction="out"/>
<pin name="!VB_CS5!/A23" direction="out"/>
<pin name="!FB_CS1" direction="out"/>
<pin name="!FB_CS0" direction="out"/>
<pin name="SD_VDD@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="EVDD@7" direction="pwr"/>
<pin name="U1RXD" direction="in"/>
<pin name="U1TXD" direction="out"/>
<pin name="!U1RTS" direction="out"/>
<pin name="!U1CTS" direction="in"/>
<pin name="FEC_COL" direction="in"/>
<pin name="FEC_CRS" direction="in"/>
<pin name="FEC_RXCLK" direction="in"/>
<pin name="FEC_RXDV" direction="in"/>
<pin name="FEC_RXD3" direction="in"/>
<pin name="FEC_RXD2" direction="in"/>
<pin name="FEC_RXD1" direction="in"/>
<pin name="FEC_RXD0" direction="in"/>
<pin name="FEC_RXER" direction="in"/>
<pin name="FEC_TXCLK" direction="in"/>
<pin name="FEC_TXEN" direction="out"/>
<pin name="FEC_TXER" direction="out"/>
<pin name="IVDD@5" direction="pwr"/>
<pin name="FEC_TXD3" direction="out"/>
<pin name="FEC_TXD2" direction="out"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="EVDD@8" direction="pwr"/>
</symbol>
<symbol name="MCF537X-CONTROL">
<pin name="DT2IN" direction="in"/>
<pin name="DT3IN" direction="in"/>
<pin name="DT1IN" direction="in"/>
<pin name="DT0IN" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="!IRQ5" direction="in"/>
<pin name="!IRQ6" direction="in"/>
<pin name="!IRQ7" direction="in"/>
<pin name="JTAG_EN" direction="in"/>
<pin name="!IRQ1" direction="in"/>
<pin name="!IRQ2" direction="in"/>
<pin name="!IRQ3" direction="in"/>
<pin name="!IRQ4" direction="in"/>
<pin name="DRAMSEL" direction="in"/>
<pin name="DSCLK" direction="in"/>
<pin name="DSI" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="XTAL" direction="out"/>
<pin name="DDATA3" direction="out"/>
<pin name="PST3" direction="out"/>
<pin name="DSO" direction="out"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="!BKPT" direction="in"/>
<pin name="EXTAL" direction="in"/>
<pin name="DDATA2" direction="out"/>
<pin name="PST2" direction="out"/>
<pin name="FB_CLK" direction="out"/>
<pin name="PSTCLK" direction="out"/>
<pin name="DDATA1" direction="out"/>
<pin name="PST1" direction="out"/>
<pin name="XTAL32K" direction="out"/>
<pin name="!RCON" direction="in"/>
<pin name="DDATA0" direction="out"/>
<pin name="PST0" direction="out"/>
<pin name="EXTAL32K" direction="in"/>
</symbol>
<symbol name="MCF537X-FLEXBUS">
<pin name="A23" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D30"/>
<pin name="D31"/>
<pin name="D26"/>
<pin name="D27"/>
<pin name="D28"/>
<pin name="D29"/>
<pin name="D24"/>
<pin name="D25"/>
<pin name="D19"/>
<pin name="D7"/>
<pin name="D3"/>
<pin name="D6"/>
<pin name="D2"/>
<pin name="D23"/>
<pin name="D20"/>
<pin name="D17"/>
<pin name="D5"/>
<pin name="D1"/>
<pin name="D22"/>
<pin name="D21"/>
<pin name="D18"/>
<pin name="D16"/>
<pin name="D4"/>
<pin name="D0"/>
<pin name="!TA" direction="in"/>
<pin name="!BE/BWE1" direction="out"/>
<pin name="!BE/BWE3" direction="out"/>
<pin name="R/!W" direction="out"/>
<pin name="!BE/BWE2" direction="out"/>
<pin name="!OE" direction="out"/>
<pin name="!BE/BWE0" direction="out"/>
<pin name="!TS" direction="out"/>
</symbol>
<symbol name="MCF537X-SDRAM">
<pin name="!FB_CS2" direction="out"/>
<pin name="!FB_CS3" direction="out"/>
<pin name="!FB_CS0" direction="out"/>
<pin name="!FB_CS4" direction="out"/>
<pin name="!FB_CS1" direction="out"/>
<pin name="!FB_CS5" direction="out"/>
<pin name="!SD_WE" direction="out"/>
<pin name="!SD_CS0" direction="out"/>
<pin name="SD_CKE" direction="out"/>
<pin name="SD_DQS3" direction="out"/>
<pin name="SD_CLK" direction="out"/>
<pin name="SD_SDR_DQS" direction="out"/>
<pin name="!SD_CLK" direction="out"/>
<pin name="SD_A10" direction="out"/>
<pin name="!SD_SCAS" direction="out"/>
<pin name="!SD_SRAS" direction="out"/>
<pin name="SD_DQS2" direction="out"/>
</symbol>
<symbol name="MCF537X-FEC">
<pin name="FEC_MDIO"/>
<pin name="FEC_TXER" direction="out"/>
<pin name="FEC_TXCLK" direction="in"/>
<pin name="FEC_RXD1" direction="in"/>
<pin name="FEC_RXCLK" direction="in"/>
<pin name="FEC_CRS" direction="in"/>
<pin name="FEC_MDC" direction="out"/>
<pin name="FEC_TXD1" direction="out"/>
<pin name="FEC_TXEN" direction="out"/>
<pin name="FEC_RXD0" direction="in"/>
<pin name="FEC_RXDV" direction="in"/>
<pin name="FEC_COL" direction="in"/>
<pin name="FEC_TXD0" direction="out"/>
<pin name="FEC_TXD2" direction="out"/>
<pin name="FEC_RXER" direction="in"/>
<pin name="FEC_RXD3" direction="in"/>
<pin name="FEC_TXD3" direction="out"/>
<pin name="FEC_RXD2" direction="in"/>
</symbol>
<symbol name="MCF537X-IO">
<pin name="U1TXD" direction="out"/>
<pin name="U1RXD" direction="in"/>
<pin name="U1CTS" direction="in"/>
<pin name="U1RTS" direction="out"/>
<pin name="I2C_SCL2"/>
<pin name="I2C_SDA2"/>
<pin name="PWM3"/>
<pin name="PWM5"/>
<pin name="PWM7"/>
<pin name="PWM1"/>
<pin name="USBOTG_P"/>
<pin name="USBOTG_M"/>
<pin name="USBHOST_P"/>
<pin name="USBHOST_M"/>
<pin name="U0RTS" direction="out"/>
<pin name="U0CTS" direction="in"/>
<pin name="U0TXD" direction="out"/>
<pin name="U0RXD" direction="in"/>
<pin name="QSPI_CS0" direction="out"/>
<pin name="QSPI_CS1" direction="out"/>
<pin name="QSPI_DOUT" direction="out"/>
<pin name="QSPI_CS2" direction="out"/>
<pin name="QSPI_DIN" direction="in"/>
<pin name="QSPI_CLK" direction="out"/>
</symbol>
<symbol name="MCF537X-PWR">
<pin name="IVDD@1" direction="pwr"/>
<pin name="EVDD@1" direction="pwr"/>
<pin name="EVDD@2" direction="pwr"/>
<pin name="SD_VDD@1" direction="pwr"/>
<pin name="SD_VDD@2" direction="pwr"/>
<pin name="EVDD@3" direction="pwr"/>
<pin name="EVDD@4" direction="pwr"/>
<pin name="EVDD@5" direction="pwr"/>
<pin name="SD_VDD@3" direction="pwr"/>
<pin name="SD_VDD@4" direction="pwr"/>
<pin name="SD_VDD@5" direction="pwr"/>
<pin name="EVDD@6" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="SD_VDD@10" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="EVDD@7" direction="pwr"/>
<pin name="PLL_VSS" direction="pwr"/>
<pin name="USB_VDD" direction="pwr"/>
<pin name="SD_VDD@6" direction="pwr"/>
<pin name="SD_VDD@7" direction="pwr"/>
<pin name="SD_VDD@8" direction="pwr"/>
<pin name="SD_VDD@9" direction="pwr"/>
<pin name="EVDD@8" direction="pwr"/>
<pin name="IVDD@2" direction="pwr"/>
<pin name="PLL_VDD" direction="pwr"/>
<pin name="IVDD@3" direction="pwr"/>
<pin name="SD_VDD@11" direction="pwr"/>
<pin name="SD_VDD@12" direction="pwr"/>
<pin name="EVDD@9" direction="pwr"/>
<pin name="EVDD@10" direction="pwr"/>
<pin name="IVDD@4" direction="pwr"/>
<pin name="USB_VSS" direction="pwr"/>
</symbol>
<symbol name="MC9S12XF-144">
<pin name="PP1-PMF1"/>
<pin name="PP0-PMF0"/>
<pin name="PD3-DATA3"/>
<pin name="PD2-DATA2"/>
<pin name="PD1-DATA1"/>
<pin name="PD0-DATA0"/>
<pin name="PT0-IOC0"/>
<pin name="PT1-IOC1"/>
<pin name="PT2-IOC2"/>
<pin name="PT3-IOC3"/>
<pin name="PJ0-IS0"/>
<pin name="PJ1-IS1"/>
<pin name="PJ2-IS2"/>
<pin name="VDDF" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSSX@3" direction="pwr"/>
<pin name="VDDX@3" direction="pwr"/>
<pin name="PT4-IOC4"/>
<pin name="PT5-IOC5"/>
<pin name="PT6-IOC6"/>
<pin name="PT7-IOC7"/>
<pin name="PC0-DATA8"/>
<pin name="PC1-DATA9"/>
<pin name="PC2-DATA10"/>
<pin name="PC3-DATA11"/>
<pin name="PC4-DATA12"/>
<pin name="PC5-DATA13"/>
<pin name="PC6-DATA14"/>
<pin name="PC7-DATA15"/>
<pin name="PJ3-STB0"/>
<pin name="PJ4-STB1"/>
<pin name="PJ5-STB2"/>
<pin name="PJ6-STB3"/>
<pin name="PJ7"/>
<pin name="PB0-ADDR0"/>
<pin name="PB1-ADDR1"/>
<pin name="PB2-ADDR2"/>
<pin name="PB3-ADDR3"/>
<pin name="BKGD-MODC"/>
<pin name="PE7-XCLKS"/>
<pin name="PE6-MODB"/>
<pin name="PE5-MODA"/>
<pin name="PE4-ECLK"/>
<pin name="PE3-LSTRB"/>
<pin name="PE2-RW"/>
<pin name="PH4-RXD_B"/>
<pin name="PH5-TXD_B"/>
<pin name="PH6-TXE_B"/>
<pin name="PH7"/>
<pin name="VDDX@2" direction="pwr"/>
<pin name="VSSX@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDDR" direction="pwr"/>
<pin name="RESET"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="EXTAL" direction="pas"/>
<pin name="XTAL" direction="pas"/>
<pin name="TEST" direction="in"/>
<pin name="PB4-ADDR4"/>
<pin name="PB5-ADDR5"/>
<pin name="PB6-ADDR6"/>
<pin name="PB7-ADDR7"/>
<pin name="PA0-ADDR8"/>
<pin name="PA1-ADDR9"/>
<pin name="PA2-ADDR10"/>
<pin name="PA3-ADDR11"/>
<pin name="VDDX@4" direction="pwr"/>
<pin name="VSSX@4" direction="pwr"/>
<pin name="PE1-IRQ" direction="in"/>
<pin name="PE0-XIRQ" direction="in"/>
<pin name="PH0-RXD_A"/>
<pin name="PH1-TXD_A"/>
<pin name="PH2-TXE_A"/>
<pin name="PH3"/>
<pin name="PK0-ADDR16"/>
<pin name="PK1-ADDR17"/>
<pin name="PK2-ADDR18"/>
<pin name="PK3-ADDR19"/>
<pin name="PK4-ADDR20"/>
<pin name="PK5-ADDR21"/>
<pin name="PK6-ADDR22"/>
<pin name="PK7-EWAIT"/>
<pin name="PA4-ADDR12"/>
<pin name="PA5-ADDR13"/>
<pin name="PA6-ADDR14"/>
<pin name="PA7-ADDR15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSSQ2" direction="pwr"/>
<pin name="PAD00-AN0"/>
<pin name="PAD08-AN8"/>
<pin name="PAD01-AN1"/>
<pin name="PAD09-AN9"/>
<pin name="PAD02-AN2"/>
<pin name="PAD10-AN10"/>
<pin name="PAD03-AN3"/>
<pin name="PAD11-AN11"/>
<pin name="PAD04-AN4"/>
<pin name="PAD12-AN12"/>
<pin name="PAD05-AN5"/>
<pin name="PAD13-AN13"/>
<pin name="PAD06-AN6"/>
<pin name="PAD14-AN14"/>
<pin name="PAD07-AN7"/>
<pin name="PAD15-AN15"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VRH" direction="pwr"/>
<pin name="VRL" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="PS0-RXD0"/>
<pin name="PS1-TXD0"/>
<pin name="PS2-RXD1"/>
<pin name="PS3-TXD1"/>
<pin name="PS4-MISO0"/>
<pin name="PS5-MOSI0"/>
<pin name="PS6-SCK0"/>
<pin name="PS7-SS0"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="PM7-SS1"/>
<pin name="PM6-SCK1"/>
<pin name="PM5-MOSI1"/>
<pin name="PM4-MISO1"/>
<pin name="PM3-FAULT3"/>
<pin name="PM2-FAULT2"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="PM1-TXCAN0"/>
<pin name="PM0-RXCAN0"/>
<pin name="VSSX@1" direction="pwr"/>
<pin name="VDDX@1" direction="pwr"/>
<pin name="PD7-DATA7"/>
<pin name="PD6-DATA6"/>
<pin name="PD5-DATA5"/>
<pin name="PD4-DATA4"/>
<pin name="PP7-FAULT1"/>
<pin name="PP6-FAULT0"/>
<pin name="PP5-PMF5"/>
<pin name="PP4-PMF4"/>
<pin name="PP3-PMF3"/>
<pin name="PP2-PMF2"/>
</symbol>
<symbol name="MC9S12XF-112">
<pin name="PP1-PMF1"/>
<pin name="PP0-PMF0"/>
<pin name="PD3-DATA3"/>
<pin name="PD2-DATA2"/>
<pin name="PD1-DATA1"/>
<pin name="PD0-DATA0"/>
<pin name="PT0-IOC0"/>
<pin name="PT1-IOC1"/>
<pin name="PT2-IOC2"/>
<pin name="PT3-IOC3"/>
<pin name="PJ0-IS0"/>
<pin name="PJ1-IS1"/>
<pin name="PJ2-IS2"/>
<pin name="VDDF5" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSSX@3" direction="pwr"/>
<pin name="VDDX@3" direction="pwr"/>
<pin name="PT4-IOC4"/>
<pin name="PT5-IOC5"/>
<pin name="PT6-IOC6"/>
<pin name="PT7-IOC7"/>
<pin name="PJ3-STB0"/>
<pin name="PJ4-STB1"/>
<pin name="PJ5-STB2"/>
<pin name="PJ6-STB3"/>
<pin name="PJ7"/>
<pin name="PB0-ADDR0"/>
<pin name="PB1-ADDR1"/>
<pin name="BKGD-MODC"/>
<pin name="PE7-XCLKS"/>
<pin name="PE6-MODB"/>
<pin name="PE5-MODA"/>
<pin name="PE4-ECLK"/>
<pin name="PE3-LSTRB"/>
<pin name="PE2-RW"/>
<pin name="PH4-RXD_B"/>
<pin name="PH5-TXD_B"/>
<pin name="PH6-TXE_B"/>
<pin name="PH7"/>
<pin name="VDDX@2" direction="pwr"/>
<pin name="VSSX@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDDR" direction="pwr"/>
<pin name="RESET"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="EXTAL" direction="pas"/>
<pin name="XTAL" direction="pas"/>
<pin name="TEST" direction="in"/>
<pin name="PA0-ADDR8"/>
<pin name="PA1-ADDR9"/>
<pin name="PA2-ADDR10"/>
<pin name="PA3-ADDR11"/>
<pin name="PE1-IRQ" direction="in"/>
<pin name="PE0-XIRQ" direction="in"/>
<pin name="PH0-RXD_A"/>
<pin name="PH1-TXD_A"/>
<pin name="PH2-TXE_A"/>
<pin name="PH3"/>
<pin name="PA4-ADDR12"/>
<pin name="PA5-ADDR13"/>
<pin name="PA6-ADDR14"/>
<pin name="PA7-ADDR15"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="PAD00-AN0"/>
<pin name="PAD08-AN8"/>
<pin name="PAD01-AN1"/>
<pin name="PAD09-AN9"/>
<pin name="PAD02-AN2"/>
<pin name="PAD10-AN10"/>
<pin name="PAD03-AN3"/>
<pin name="PAD11-AN11"/>
<pin name="PAD04-AN4"/>
<pin name="PAD12-AN12"/>
<pin name="PAD05-AN5"/>
<pin name="PAD13-AN13"/>
<pin name="PAD06-AN6"/>
<pin name="PAD14-AN14"/>
<pin name="PAD07-AN7"/>
<pin name="PAD15-AN15"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VRH" direction="pwr"/>
<pin name="VRL" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PS0-RXD0"/>
<pin name="PS1-TXD0"/>
<pin name="PS2-RXD1"/>
<pin name="PS3-TXD1"/>
<pin name="PS4-MISO0"/>
<pin name="PS5-MOSI0"/>
<pin name="PS6-SCK0"/>
<pin name="PS7-SS0"/>
<pin name="PM7-SS1"/>
<pin name="PM6-SCK1"/>
<pin name="PM5-MOSI1"/>
<pin name="PM4-MISO1"/>
<pin name="PM3-FAULT3"/>
<pin name="PM2-FAULT2"/>
<pin name="PM1-TXCAN0"/>
<pin name="PM0-RXCAN0"/>
<pin name="VSSX@1" direction="pwr"/>
<pin name="VDDX@1" direction="pwr"/>
<pin name="PD5-DATA5"/>
<pin name="PD4-DATA4"/>
<pin name="PP7-FAULT1"/>
<pin name="PP6-FAULT0"/>
<pin name="PP5-PMF5"/>
<pin name="PP4-PMF4"/>
<pin name="PP3-PMF3"/>
<pin name="PP2-PMF2"/>
</symbol>
<symbol name="MC9S12XF-64">
<pin name="PP1-PMF1"/>
<pin name="PP0-PMF0"/>
<pin name="PT0-IOC0"/>
<pin name="PT1-IOC1"/>
<pin name="PT2-IOC2"/>
<pin name="PT3-IOC3"/>
<pin name="VDDF5" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="PT4-IOC4"/>
<pin name="PT5-IOC5"/>
<pin name="PT6-IOC6"/>
<pin name="PT7-IOC7"/>
<pin name="PJ3-STB0"/>
<pin name="PJ4-STB1"/>
<pin name="PJ5-STB2"/>
<pin name="PJ6-STB3"/>
<pin name="BKGD-MODC"/>
<pin name="PE7-XCLKS"/>
<pin name="PE4-ECLK"/>
<pin name="VDDX2" direction="pwr"/>
<pin name="VSSX2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VDDR" direction="pwr"/>
<pin name="RESET"/>
<pin name="VDDPLL" direction="pwr"/>
<pin name="NC" direction="nc"/>
<pin name="VSSPLL" direction="pwr"/>
<pin name="EXTAL" direction="pas"/>
<pin name="XTAL" direction="pas"/>
<pin name="TEST" direction="in"/>
<pin name="PE1-IRQ" direction="in"/>
<pin name="PE0-XIRQ" direction="in"/>
<pin name="PH0-RXD_A"/>
<pin name="PH1-TXD_A"/>
<pin name="PH2-TXE_A"/>
<pin name="PH3"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="PAD00-AN0"/>
<pin name="PAD01-AN1"/>
<pin name="PAD02-AN2"/>
<pin name="PAD03-AN3"/>
<pin name="PAD04-AN4"/>
<pin name="PAD05-AN5"/>
<pin name="PAD06-AN6"/>
<pin name="PAD07-AN7"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VRH" direction="pwr"/>
<pin name="VRL" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
<pin name="PS0-RXD0"/>
<pin name="PS1-TXD0"/>
<pin name="PS4-MISO0"/>
<pin name="PS5-MOSI0"/>
<pin name="PS6-SCK0"/>
<pin name="PS7-SS0"/>
<pin name="PM1-TXCAN0"/>
<pin name="PM0-RXCAN0"/>
<pin name="VSSX@1" direction="pwr"/>
<pin name="VDDX@1" direction="pwr"/>
<pin name="PP5-PMF5"/>
<pin name="PP4-PMF4"/>
<pin name="PP3-PMF3"/>
<pin name="PP2-PMF2"/>
</symbol>
<symbol name="MC33932">
<pin name="D1" direction="in"/>
<pin name="FBA" direction="out"/>
<pin name="EN/!D2" direction="in"/>
<pin name="VPWRA" direction="in"/>
<pin name="VPWRA@1" direction="in"/>
<pin name="VPWRA@2" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT1@1" direction="pas"/>
<pin name="OUT1@2" direction="pas"/>
<pin name="PGNDA" direction="pwr"/>
<pin name="PGNDA@1" direction="pwr"/>
<pin name="PGNDB" direction="pwr"/>
<pin name="PGNDB@1" direction="pwr"/>
<pin name="OUT4" direction="out"/>
<pin name="OUT4@1" direction="pas"/>
<pin name="OUT4@2" direction="pas"/>
<pin name="VPWRB" direction="in"/>
<pin name="VPWRB@1" direction="in"/>
<pin name="CCPB" direction="out"/>
<pin name="IN4" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="!SFB" direction="oc"/>
<pin name="D3" direction="in"/>
<pin name="FBB" direction="out"/>
<pin name="EN/!D4" direction="in"/>
<pin name="VPWRB@2" direction="in"/>
<pin name="VPWRB@3" direction="in"/>
<pin name="VPWRB@4" direction="in"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT3@1" direction="pas"/>
<pin name="OUT3@2" direction="pas"/>
<pin name="PGNDB@2" direction="pwr"/>
<pin name="PGNDB@3" direction="pwr"/>
<pin name="PGNDA@2" direction="pwr"/>
<pin name="PGNDA@3" direction="pwr"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT2@1" direction="pas"/>
<pin name="OUT2@2" direction="pas"/>
<pin name="VPWRA@3" direction="in"/>
<pin name="VPWRA@4" direction="in"/>
<pin name="CCPA" direction="out"/>
<pin name="IN2" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="!SFA" direction="oc"/>
<pin name="EH@1" direction="pas"/>
<pin name="EH@2" direction="pas"/>
<pin name="EH@3" direction="pas"/>
</symbol>
<symbol name="MC9S08GT16A">
<pin name="!RESET" direction="in"/>
<pin name="PTC0/TXD2"/>
<pin name="PTC1/RXD2"/>
<pin name="PTC2/SDA"/>
<pin name="PTC3/SCL"/>
<pin name="PTC4"/>
<pin name="PTC5"/>
<pin name="PTC6"/>
<pin name="PTC7"/>
<pin name="PTE0/TXD1"/>
<pin name="PTE1/RXD1"/>
<pin name="IRQ"/>
<pin name="PTE2/!SS"/>
<pin name="PTE3/MISO"/>
<pin name="PTE4/MOSI"/>
<pin name="PTE5/SPSCK"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PTD0/TPM1CLK/TPM1CH0"/>
<pin name="PTD1/TPM1CH1"/>
<pin name="PTD2/TPM1CH2"/>
<pin name="PTD3/TPM2CLK/TPM2CH0"/>
<pin name="PTD4/TPM2CH1"/>
<pin name="PTB0/ADP0"/>
<pin name="PTB1/ADP1"/>
<pin name="PTB2/ADP2"/>
<pin name="PTB3/ADP3"/>
<pin name="PTB4/ADP4"/>
<pin name="PTB5/ADP5"/>
<pin name="PTB6/ADP6"/>
<pin name="PTB7/ADP7"/>
<pin name="VREFH"/>
<pin name="VREFL"/>
<pin name="PTA0/KBIP0"/>
<pin name="PTA1/KBIP1"/>
<pin name="PTA2/KBIP2"/>
<pin name="PTA3/KBIP3"/>
<pin name="PTA4/KBIP4"/>
<pin name="PTA5/KBIP5"/>
<pin name="PTA6/KBIP6"/>
<pin name="PTA7/KBIP7"/>
<pin name="VDDAD" direction="pwr"/>
<pin name="VSSAD" direction="pwr"/>
<pin name="PTG0/BKGD/MS"/>
<pin name="PTG1/XTAL"/>
<pin name="PTG2/EXTAL"/>
<pin name="PTG3"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="MC9S08GT16A-44">
<pin name="!RESET" direction="in"/>
<pin name="PTC0/TXD2"/>
<pin name="PTC1/RXD2"/>
<pin name="PTC2/SDA"/>
<pin name="PTC3/SCL"/>
<pin name="PTC4"/>
<pin name="PTC5"/>
<pin name="PTC6"/>
<pin name="PTE0/TXD1"/>
<pin name="PTE1/RXD1"/>
<pin name="IRQ"/>
<pin name="PTE2/!SS"/>
<pin name="PTE3/MISO"/>
<pin name="PTE4/MOSI"/>
<pin name="PTE5/SPSCK"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PTD0/TPM1CLK/TPM1CH0"/>
<pin name="PTD1/TPM1CH1"/>
<pin name="PTD3/TPM2CLK/TPM2CH0"/>
<pin name="PTD4/TPM2CH1"/>
<pin name="PTB0/ADP0"/>
<pin name="PTB1/ADP1"/>
<pin name="PTB2/ADP2"/>
<pin name="PTB3/ADP3"/>
<pin name="PTB4/ADP4"/>
<pin name="PTB5/ADP5"/>
<pin name="PTB6/ADP6"/>
<pin name="PTB7/ADP7"/>
<pin name="VREFH"/>
<pin name="VREFL"/>
<pin name="PTA0/KBIP0"/>
<pin name="PTA1/KBIP1"/>
<pin name="PTA2/KBIP2"/>
<pin name="PTA3/KBIP3"/>
<pin name="PTA4/KBIP4"/>
<pin name="PTA5/KBIP5"/>
<pin name="PTA6/KBIP6"/>
<pin name="PTA7/KBIP7"/>
<pin name="VDDAD" direction="pwr"/>
<pin name="VSSAD" direction="pwr"/>
<pin name="PTG0/BKGD/MS"/>
<pin name="PTG1/XTAL"/>
<pin name="PTG2/EXTAL"/>
</symbol>
<symbol name="MC9S08GT16A-42">
<pin name="!RESET" direction="in"/>
<pin name="PTC0/TXD2"/>
<pin name="PTC1/RXD2"/>
<pin name="PTC2/SDA"/>
<pin name="PTC3/SCL"/>
<pin name="PTC4"/>
<pin name="PTE0/TXD1"/>
<pin name="PTE1/RXD1"/>
<pin name="IRQ"/>
<pin name="PTE2/!SS"/>
<pin name="PTE3/MISO"/>
<pin name="PTE4/MOSI"/>
<pin name="PTE5/SPSCK"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PTD0/TPM1CLK/TPM1CH0"/>
<pin name="PTD1/TPM1CH1"/>
<pin name="PTD3/TPM2CLK/TPM2CH0"/>
<pin name="PTD4/TPM2CH1"/>
<pin name="PTB0/ADP0"/>
<pin name="PTB1/ADP1"/>
<pin name="PTB2/ADP2"/>
<pin name="PTB3/ADP3"/>
<pin name="PTB4/ADP4"/>
<pin name="PTB5/ADP5"/>
<pin name="PTB6/ADP6"/>
<pin name="PTB7/ADP7"/>
<pin name="VREFH"/>
<pin name="VREFL"/>
<pin name="PTA0/KBIP0"/>
<pin name="PTA1/KBIP1"/>
<pin name="PTA2/KBIP2"/>
<pin name="PTA3/KBIP3"/>
<pin name="PTA4/KBIP4"/>
<pin name="PTA5/KBIP5"/>
<pin name="PTA6/KBIP6"/>
<pin name="PTA7/KBIP7"/>
<pin name="VDDAD" direction="pwr"/>
<pin name="VSSAD" direction="pwr"/>
<pin name="PTG0/BKGD/MS"/>
<pin name="PTG1/XTAL"/>
<pin name="PTG2/EXTAL"/>
</symbol>
<symbol name="MC9S08GT16A-32">
<pin name="!RESET" direction="in"/>
<pin name="PTC0/TXD2"/>
<pin name="PTC1/RXD2"/>
<pin name="PTC2/SDA"/>
<pin name="PTC3/SCL"/>
<pin name="PTE0/TXD1"/>
<pin name="PTE1/RXD1"/>
<pin name="IRQ"/>
<pin name="PTE2/!SS"/>
<pin name="PTE3/MISO"/>
<pin name="PTE4/MOSI"/>
<pin name="PTE5/SPSCK"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="PTD0/TPM1CLK/TPM1CH0"/>
<pin name="PTD1/TPM1CH1"/>
<pin name="PTD3/TPM2CLK/TPM2CH0"/>
<pin name="PTB0/ADP0"/>
<pin name="PTB1/ADP1"/>
<pin name="PTB2/ADP2"/>
<pin name="PTB3/ADP3"/>
<pin name="VREFH"/>
<pin name="VREFL"/>
<pin name="PTA4/KBIP4"/>
<pin name="PTA5/KBIP5"/>
<pin name="PTA6/KBIP6"/>
<pin name="PTA7/KBIP7"/>
<pin name="VDDAD" direction="pwr"/>
<pin name="VSSAD" direction="pwr"/>
<pin name="PTG0/BKGD/MS"/>
<pin name="PTG1/XTAL"/>
<pin name="PTG2/EXTAL"/>
<pin name="EXP" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FSA95601" prefix="IC">
<description>&lt;b&gt;Digital Audio Amplifier Controller&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/dsp/doc/prod_brief/FSA95601PB.pdf</description>
<gates>
<gate name="G$1" symbol="FSA95601"/>
</gates>
<devices>
<device name="" package="QFP-12X12-80E">
<connects>
<connect gate="G$1" pin="CAPDIGP" pad="13"/>
<connect gate="G$1" pin="CAPVCOM" pad="38"/>
<connect gate="G$1" pin="CAPVCOP" pad="37"/>
<connect gate="G$1" pin="CLKOUTM" pad="32"/>
<connect gate="G$1" pin="CLKOUTP" pad="31"/>
<connect gate="G$1" pin="CSB_A1" pad="25"/>
<connect gate="G$1" pin="FDBKCH0A" pad="57"/>
<connect gate="G$1" pin="FDBKCH0B" pad="56"/>
<connect gate="G$1" pin="FDBKCH1A" pad="54"/>
<connect gate="G$1" pin="FDBKCH1B" pad="53"/>
<connect gate="G$1" pin="FDBKCH2A" pad="52"/>
<connect gate="G$1" pin="FDBKCH2B" pad="51"/>
<connect gate="G$1" pin="FDBKCH3A" pad="50"/>
<connect gate="G$1" pin="FDBKCH3B" pad="49"/>
<connect gate="G$1" pin="FDBKCH4A" pad="48"/>
<connect gate="G$1" pin="FDBKCH4B" pad="47"/>
<connect gate="G$1" pin="FDBKCH5A" pad="45"/>
<connect gate="G$1" pin="FDBKCH5B" pad="44"/>
<connect gate="G$1" pin="I2C_SPIB_MUTEB" pad="26"/>
<connect gate="G$1" pin="IRQB" pad="14"/>
<connect gate="G$1" pin="LRCLK" pad="19"/>
<connect gate="G$1" pin="MISO_SDA" pad="21"/>
<connect gate="G$1" pin="MOSI_A0" pad="20"/>
<connect gate="G$1" pin="PWMCH0AHI" pad="10"/>
<connect gate="G$1" pin="PWMCH0ALO" pad="9"/>
<connect gate="G$1" pin="PWMCH0BHI" pad="6"/>
<connect gate="G$1" pin="PWMCH0BLO" pad="7"/>
<connect gate="G$1" pin="PWMCH1AHI" pad="4"/>
<connect gate="G$1" pin="PWMCH1ALO" pad="3"/>
<connect gate="G$1" pin="PWMCH1BHI" pad="80"/>
<connect gate="G$1" pin="PWMCH1BLO" pad="1"/>
<connect gate="G$1" pin="PWMCH2AHI" pad="79"/>
<connect gate="G$1" pin="PWMCH2ALO" pad="78"/>
<connect gate="G$1" pin="PWMCH2BHI" pad="75"/>
<connect gate="G$1" pin="PWMCH2BLO" pad="76"/>
<connect gate="G$1" pin="PWMCH3AHI" pad="73"/>
<connect gate="G$1" pin="PWMCH3ALO" pad="72"/>
<connect gate="G$1" pin="PWMCH3BHI" pad="69"/>
<connect gate="G$1" pin="PWMCH3BLO" pad="70"/>
<connect gate="G$1" pin="PWMCH4AHI" pad="68"/>
<connect gate="G$1" pin="PWMCH4ALO" pad="67"/>
<connect gate="G$1" pin="PWMCH4BHI" pad="64"/>
<connect gate="G$1" pin="PWMCH4BLO" pad="65"/>
<connect gate="G$1" pin="PWMCH5AHI" pad="62"/>
<connect gate="G$1" pin="PWMCH5ALO" pad="61"/>
<connect gate="G$1" pin="PWMCH5BHI" pad="58"/>
<connect gate="G$1" pin="PWMCH5BLO" pad="59"/>
<connect gate="G$1" pin="PWMREF" pad="42"/>
<connect gate="G$1" pin="PWRDNB" pad="28"/>
<connect gate="G$1" pin="RESETB" pad="27"/>
<connect gate="G$1" pin="SCK_SCL" pad="24"/>
<connect gate="G$1" pin="SCLK" pad="18"/>
<connect gate="G$1" pin="SDIN0" pad="15"/>
<connect gate="G$1" pin="SDIN1" pad="16"/>
<connect gate="G$1" pin="SDIN2" pad="17"/>
<connect gate="G$1" pin="TESTEN" pad="29"/>
<connect gate="G$1" pin="VDDA2" pad="39"/>
<connect gate="G$1" pin="VDDADC" pad="30"/>
<connect gate="G$1" pin="VDDCLK" pad="40"/>
<connect gate="G$1" pin="VDDD" pad="11"/>
<connect gate="G$1" pin="VDDDIO" pad="22"/>
<connect gate="G$1" pin="VDDINT" pad="43"/>
<connect gate="G$1" pin="VDDIOCH01" pad="5"/>
<connect gate="G$1" pin="VDDIOCH23" pad="74"/>
<connect gate="G$1" pin="VDDIOCH45" pad="63"/>
<connect gate="G$1" pin="VDDOSC" pad="36"/>
<connect gate="G$1" pin="VREF" pad="41"/>
<connect gate="G$1" pin="VSSD" pad="12"/>
<connect gate="G$1" pin="VSSDIO" pad="23"/>
<connect gate="G$1" pin="VSSIOCH0" pad="8"/>
<connect gate="G$1" pin="VSSIOCH1" pad="2"/>
<connect gate="G$1" pin="VSSIOCH2" pad="77"/>
<connect gate="G$1" pin="VSSIOCH3" pad="71"/>
<connect gate="G$1" pin="VSSIOCH4" pad="66"/>
<connect gate="G$1" pin="VSSIOCH5" pad="60"/>
<connect gate="G$1" pin="VSSSH2" pad="55"/>
<connect gate="G$1" pin="VSSSH7" pad="46"/>
<connect gate="G$1" pin="VSS_EXP" pad="EXP"/>
<connect gate="G$1" pin="XTAL1" pad="33"/>
<connect gate="G$1" pin="XTAL2" pad="34"/>
<connect gate="G$1" pin="XTALGND" pad="35"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="FSA95601AH"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="69M3598"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68HC908AP*" prefix="IC">
<description>&lt;b&gt;8-bit microcontroller units (MCUs)&lt;/b&gt; low-cost, high-performance M68HC08 Family&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC68HC908AP64.pdf</description>
<gates>
<gate name="G$1" symbol="68HC908AP8_V2"/>
</gates>
<devices>
<device name="FA" package="TQFP48_7X7">
<connects>
<connect gate="G$1" pin="!IRQ1" pad="9"/>
<connect gate="G$1" pin="!RST" pad="11"/>
<connect gate="G$1" pin="CGMXFC" pad="48"/>
<connect gate="G$1" pin="OSC1" pad="5"/>
<connect gate="G$1" pin="OSC2" pad="6"/>
<connect gate="G$1" pin="PTA0/ADC0" pad="32"/>
<connect gate="G$1" pin="PTA1/ADC1" pad="30"/>
<connect gate="G$1" pin="PTA2/ADC2" pad="29"/>
<connect gate="G$1" pin="PTA3/ADC3" pad="28"/>
<connect gate="G$1" pin="PTA4/ADC4" pad="27"/>
<connect gate="G$1" pin="PTA5/ADC5" pad="26"/>
<connect gate="G$1" pin="PTA6/ADC6" pad="25"/>
<connect gate="G$1" pin="PTA7/ADC7" pad="23"/>
<connect gate="G$1" pin="PTB0/SDA" pad="14"/>
<connect gate="G$1" pin="PTB1/SCL" pad="13"/>
<connect gate="G$1" pin="PTB2/TXD" pad="12"/>
<connect gate="G$1" pin="PTB3/RXD" pad="10"/>
<connect gate="G$1" pin="PTB4/T1CH0" pad="8"/>
<connect gate="G$1" pin="PTB5/T1CH1" pad="3"/>
<connect gate="G$1" pin="PTB6/T2CH0" pad="1"/>
<connect gate="G$1" pin="PTB7/T2CH1" pad="47"/>
<connect gate="G$1" pin="PTC0/!IRQ2" pad="22"/>
<connect gate="G$1" pin="PTC1" pad="21"/>
<connect gate="G$1" pin="PTC2/MISO" pad="20"/>
<connect gate="G$1" pin="PTC3/MOSI" pad="19"/>
<connect gate="G$1" pin="PTC4/!SS" pad="18"/>
<connect gate="G$1" pin="PTC5/SPSCK" pad="17"/>
<connect gate="G$1" pin="PTC6/SCTXD" pad="16"/>
<connect gate="G$1" pin="PTC7/SCRXD" pad="15"/>
<connect gate="G$1" pin="PTD0/KBI0" pad="46"/>
<connect gate="G$1" pin="PTD1/KBI1" pad="45"/>
<connect gate="G$1" pin="PTD2/KBI2" pad="44"/>
<connect gate="G$1" pin="PTD3/KBI3" pad="41"/>
<connect gate="G$1" pin="PTD4/KBI4" pad="40"/>
<connect gate="G$1" pin="PTD5/KBI5" pad="39"/>
<connect gate="G$1" pin="PTD6/KBI6" pad="38"/>
<connect gate="G$1" pin="PTD7/KBI7" pad="37"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VDDA" pad="43"/>
<connect gate="G$1" pin="VREFH" pad="36"/>
<connect gate="G$1" pin="VREFL" pad="35"/>
<connect gate="G$1" pin="VREG" pad="2"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="VSSA" pad="42"/>
</connects>
<technologies>
<technology name="16C">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP16CFA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88H9989"/>
</technology>
<technology name="32C">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP32CFA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="86H4494"/>
</technology>
<technology name="64C">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP64CFA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="86H4497"/>
</technology>
<technology name="8C">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP8CFA"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88H9992"/>
</technology>
</technologies>
</device>
<device name="FB" package="QFP44">
<connects>
<connect gate="G$1" pin="!IRQ1" pad="9"/>
<connect gate="G$1" pin="!RST" pad="11"/>
<connect gate="G$1" pin="CGMXFC" pad="44"/>
<connect gate="G$1" pin="OSC1" pad="5"/>
<connect gate="G$1" pin="OSC2" pad="6"/>
<connect gate="G$1" pin="PTA0/ADC0" pad="30"/>
<connect gate="G$1" pin="PTA1/ADC1" pad="29"/>
<connect gate="G$1" pin="PTA2/ADC2" pad="28"/>
<connect gate="G$1" pin="PTA3/ADC3" pad="27"/>
<connect gate="G$1" pin="PTA4/ADC4" pad="26"/>
<connect gate="G$1" pin="PTA5/ADC5" pad="25"/>
<connect gate="G$1" pin="PTA6/ADC6" pad="24"/>
<connect gate="G$1" pin="PTA7/ADC7" pad="23"/>
<connect gate="G$1" pin="PTB0/SDA" pad="14"/>
<connect gate="G$1" pin="PTB1/SCL" pad="13"/>
<connect gate="G$1" pin="PTB2/TXD" pad="12"/>
<connect gate="G$1" pin="PTB3/RXD" pad="10"/>
<connect gate="G$1" pin="PTB4/T1CH0" pad="8"/>
<connect gate="G$1" pin="PTB5/T1CH1" pad="3"/>
<connect gate="G$1" pin="PTB6/T2CH0" pad="1"/>
<connect gate="G$1" pin="PTB7/T2CH1" pad="43"/>
<connect gate="G$1" pin="PTC0/!IRQ2" pad="22"/>
<connect gate="G$1" pin="PTC1" pad="21"/>
<connect gate="G$1" pin="PTC2/MISO" pad="20"/>
<connect gate="G$1" pin="PTC3/MOSI" pad="19"/>
<connect gate="G$1" pin="PTC4/!SS" pad="18"/>
<connect gate="G$1" pin="PTC5/SPSCK" pad="17"/>
<connect gate="G$1" pin="PTC6/SCTXD" pad="16"/>
<connect gate="G$1" pin="PTC7/SCRXD" pad="15"/>
<connect gate="G$1" pin="PTD0/KBI0" pad="42"/>
<connect gate="G$1" pin="PTD1/KBI1" pad="41"/>
<connect gate="G$1" pin="PTD2/KBI2" pad="40"/>
<connect gate="G$1" pin="PTD3/KBI3" pad="37"/>
<connect gate="G$1" pin="PTD4/KBI4" pad="36"/>
<connect gate="G$1" pin="PTD5/KBI5" pad="35"/>
<connect gate="G$1" pin="PTD6/KBI6" pad="34"/>
<connect gate="G$1" pin="PTD7/KBI7" pad="33"/>
<connect gate="G$1" pin="VDD" pad="4"/>
<connect gate="G$1" pin="VDDA" pad="39"/>
<connect gate="G$1" pin="VREFH" pad="32"/>
<connect gate="G$1" pin="VREFL" pad="31"/>
<connect gate="G$1" pin="VREG" pad="2"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="VSSA" pad="38"/>
</connects>
<technologies>
<technology name="16C">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP16CFB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88H9990"/>
</technology>
<technology name="23C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="64C">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP64CFB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="86H4498"/>
</technology>
<technology name="8C">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP8CFB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88H9993"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="68HC908AP*CB" prefix="IC">
<description>&lt;b&gt;8-bit microcontroller units (MCUs)&lt;/b&gt; low-cost, high-performance M68HC08 Family&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC68HC908AP64.pdf</description>
<gates>
<gate name="G$1" symbol="68HC908AP8_V1"/>
</gates>
<devices>
<device name="" package="PSDIP_42">
<connects>
<connect gate="G$1" pin="!IRQ1" pad="14"/>
<connect gate="G$1" pin="!RST" pad="16"/>
<connect gate="G$1" pin="CGMXFC" pad="5"/>
<connect gate="G$1" pin="OSC1" pad="10"/>
<connect gate="G$1" pin="OSC2" pad="11"/>
<connect gate="G$1" pin="PRB3/RXD" pad="15"/>
<connect gate="G$1" pin="PTA0/ADC0" pad="33"/>
<connect gate="G$1" pin="PTA1/ADC1" pad="32"/>
<connect gate="G$1" pin="PTA2/ADC2" pad="31"/>
<connect gate="G$1" pin="PTA3/ADC3" pad="30"/>
<connect gate="G$1" pin="PTA4/ADC4" pad="29"/>
<connect gate="G$1" pin="PTA5/ADC5" pad="28"/>
<connect gate="G$1" pin="PTA6/ADC6" pad="27"/>
<connect gate="G$1" pin="PTA7/ADC7" pad="26"/>
<connect gate="G$1" pin="PTB0/SDA" pad="19"/>
<connect gate="G$1" pin="PTB1/SCL" pad="18"/>
<connect gate="G$1" pin="PTB2/TXD" pad="17"/>
<connect gate="G$1" pin="PTB4/T1CH0" pad="13"/>
<connect gate="G$1" pin="PTB5/T2CH1" pad="8"/>
<connect gate="G$1" pin="PTB6/T2CH0" pad="6"/>
<connect gate="G$1" pin="PTB7/T2CH1" pad="3"/>
<connect gate="G$1" pin="PTC2/MISO" pad="25"/>
<connect gate="G$1" pin="PTC3/MOSI" pad="24"/>
<connect gate="G$1" pin="PTC4/!SS" pad="23"/>
<connect gate="G$1" pin="PTC5/SPSCK" pad="22"/>
<connect gate="G$1" pin="PTC6/SCTXD" pad="21"/>
<connect gate="G$1" pin="PTC7/SCRXD" pad="20"/>
<connect gate="G$1" pin="PTD0/KBI0" pad="4"/>
<connect gate="G$1" pin="PTD1/KBI1" pad="2"/>
<connect gate="G$1" pin="PTD2/KBI2" pad="1"/>
<connect gate="G$1" pin="PTD3/KBI3" pad="40"/>
<connect gate="G$1" pin="PTD4/KBI4" pad="39"/>
<connect gate="G$1" pin="PTD5/KBI5" pad="38"/>
<connect gate="G$1" pin="PTD6/KBI6" pad="37"/>
<connect gate="G$1" pin="PTD7/KBI7" pad="36"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VDDA" pad="42"/>
<connect gate="G$1" pin="VREFH" pad="35"/>
<connect gate="G$1" pin="VREFL" pad="34"/>
<connect gate="G$1" pin="VREG" pad="7"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSSA" pad="41"/>
</connects>
<technologies>
<technology name="16">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP16CB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88H9988"/>
</technology>
<technology name="32">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP32CB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="86H4493"/>
</technology>
<technology name="64">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP64CB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="86H4496"/>
</technology>
<technology name="8">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC68HC908AP8CB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="88H9991"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCF537*" prefix="IC">
<description>&lt;b&gt;MCF537x ColdFire® Microprocessor&lt;/b&gt;&lt;p&gt;
Source: www.freescale.com .. MCF5373DS.pdf</description>
<gates>
<gate name="G$1" symbol="MCF5372CAB180"/>
</gates>
<devices>
<device name="" package="QFP160">
<connects>
<connect gate="G$1" pin="!BE/BWE0" pad="56"/>
<connect gate="G$1" pin="!BE/BWE1" pad="24"/>
<connect gate="G$1" pin="!BE/BWE2" pad="54"/>
<connect gate="G$1" pin="!BE/BWE3" pad="26"/>
<connect gate="G$1" pin="!FB_CS0" pad="136"/>
<connect gate="G$1" pin="!FB_CS1" pad="135"/>
<connect gate="G$1" pin="!IRQ1" pad="100"/>
<connect gate="G$1" pin="!IRQ4" pad="101"/>
<connect gate="G$1" pin="!IRQ7" pad="102"/>
<connect gate="G$1" pin="!OE" pad="66"/>
<connect gate="G$1" pin="!RCON" pad="72"/>
<connect gate="G$1" pin="!RESET" pad="95"/>
<connect gate="G$1" pin="!RSTOUT" pad="86"/>
<connect gate="G$1" pin="!SD_CLK" pad="38"/>
<connect gate="G$1" pin="!SD_CS0" pad="15"/>
<connect gate="G$1" pin="!SD_SCAS" pad="44"/>
<connect gate="G$1" pin="!SD_SRAS" pad="45"/>
<connect gate="G$1" pin="!SD_WE" pad="13"/>
<connect gate="G$1" pin="!TA" pad="106"/>
<connect gate="G$1" pin="!TRST!/DSCLK" pad="88"/>
<connect gate="G$1" pin="!TS" pad="12"/>
<connect gate="G$1" pin="!U0CTS" pad="85"/>
<connect gate="G$1" pin="!U0RTS" pad="84"/>
<connect gate="G$1" pin="!U1CTS" pad="143"/>
<connect gate="G$1" pin="!U1RTS" pad="142"/>
<connect gate="G$1" pin="!VB_CS4!/A22" pad="133"/>
<connect gate="G$1" pin="!VB_CS5!/A23" pad="134"/>
<connect gate="G$1" pin="A0" pad="107"/>
<connect gate="G$1" pin="A1" pad="108"/>
<connect gate="G$1" pin="A10" pad="117"/>
<connect gate="G$1" pin="A11" pad="118"/>
<connect gate="G$1" pin="A12" pad="119"/>
<connect gate="G$1" pin="A13" pad="120"/>
<connect gate="G$1" pin="A14" pad="123"/>
<connect gate="G$1" pin="A15" pad="126"/>
<connect gate="G$1" pin="A16" pad="127"/>
<connect gate="G$1" pin="A17" pad="128"/>
<connect gate="G$1" pin="A18" pad="129"/>
<connect gate="G$1" pin="A19" pad="130"/>
<connect gate="G$1" pin="A2" pad="109"/>
<connect gate="G$1" pin="A20" pad="131"/>
<connect gate="G$1" pin="A21" pad="132"/>
<connect gate="G$1" pin="A3" pad="110"/>
<connect gate="G$1" pin="A4" pad="111"/>
<connect gate="G$1" pin="A5" pad="112"/>
<connect gate="G$1" pin="A6" pad="113"/>
<connect gate="G$1" pin="A7" pad="114"/>
<connect gate="G$1" pin="A8" pad="115"/>
<connect gate="G$1" pin="A9" pad="116"/>
<connect gate="G$1" pin="ALLPST" pad="73"/>
<connect gate="G$1" pin="D0" pad="64"/>
<connect gate="G$1" pin="D1" pad="63"/>
<connect gate="G$1" pin="D10" pad="21"/>
<connect gate="G$1" pin="D11" pad="20"/>
<connect gate="G$1" pin="D12" pad="19"/>
<connect gate="G$1" pin="D13" pad="18"/>
<connect gate="G$1" pin="D14" pad="17"/>
<connect gate="G$1" pin="D15" pad="16"/>
<connect gate="G$1" pin="D16" pad="53"/>
<connect gate="G$1" pin="D17" pad="52"/>
<connect gate="G$1" pin="D18" pad="51"/>
<connect gate="G$1" pin="D19" pad="50"/>
<connect gate="G$1" pin="D2" pad="62"/>
<connect gate="G$1" pin="D20" pad="49"/>
<connect gate="G$1" pin="D21" pad="48"/>
<connect gate="G$1" pin="D22" pad="47"/>
<connect gate="G$1" pin="D23" pad="46"/>
<connect gate="G$1" pin="D24" pad="34"/>
<connect gate="G$1" pin="D25" pad="33"/>
<connect gate="G$1" pin="D26" pad="32"/>
<connect gate="G$1" pin="D27" pad="31"/>
<connect gate="G$1" pin="D28" pad="30"/>
<connect gate="G$1" pin="D29" pad="29"/>
<connect gate="G$1" pin="D3" pad="61"/>
<connect gate="G$1" pin="D30" pad="28"/>
<connect gate="G$1" pin="D31" pad="27"/>
<connect gate="G$1" pin="D4" pad="60"/>
<connect gate="G$1" pin="D5" pad="59"/>
<connect gate="G$1" pin="D6" pad="58"/>
<connect gate="G$1" pin="D7" pad="57"/>
<connect gate="G$1" pin="D8" pad="23"/>
<connect gate="G$1" pin="D9" pad="22"/>
<connect gate="G$1" pin="DRAMSEL" pad="92"/>
<connect gate="G$1" pin="DSI" pad="90"/>
<connect gate="G$1" pin="DSO" pad="74"/>
<connect gate="G$1" pin="DT0IN" pad="5"/>
<connect gate="G$1" pin="DT1IN" pad="6"/>
<connect gate="G$1" pin="DT2IN" pad="7"/>
<connect gate="G$1" pin="DT3IN" pad="8"/>
<connect gate="G$1" pin="EVDD@1" pad="9"/>
<connect gate="G$1" pin="EVDD@2" pad="69"/>
<connect gate="G$1" pin="EVDD@3" pad="71"/>
<connect gate="G$1" pin="EVDD@4" pad="81"/>
<connect gate="G$1" pin="EVDD@5" pad="94"/>
<connect gate="G$1" pin="EVDD@6" pad="103"/>
<connect gate="G$1" pin="EVDD@7" pad="139"/>
<connect gate="G$1" pin="EVDD@8" pad="160"/>
<connect gate="G$1" pin="EXTAL" pad="91"/>
<connect gate="G$1" pin="FB_CLK" pad="40"/>
<connect gate="G$1" pin="FEC_COL" pad="144"/>
<connect gate="G$1" pin="FEC_CRS" pad="145"/>
<connect gate="G$1" pin="FEC_MDC" pad="4"/>
<connect gate="G$1" pin="FEC_MDIO" pad="3"/>
<connect gate="G$1" pin="FEC_RXCLK" pad="146"/>
<connect gate="G$1" pin="FEC_RXD0" pad="151"/>
<connect gate="G$1" pin="FEC_RXD1" pad="150"/>
<connect gate="G$1" pin="FEC_RXD2" pad="149"/>
<connect gate="G$1" pin="FEC_RXD3" pad="148"/>
<connect gate="G$1" pin="FEC_RXDV" pad="147"/>
<connect gate="G$1" pin="FEC_RXER" pad="152"/>
<connect gate="G$1" pin="FEC_TXCLK" pad="153"/>
<connect gate="G$1" pin="FEC_TXD0" pad="2"/>
<connect gate="G$1" pin="FEC_TXD1" pad="1"/>
<connect gate="G$1" pin="FEC_TXD2" pad="158"/>
<connect gate="G$1" pin="FEC_TXD3" pad="157"/>
<connect gate="G$1" pin="FEC_TXEN" pad="154"/>
<connect gate="G$1" pin="FEC_TXER" pad="155"/>
<connect gate="G$1" pin="IVDD@1" pad="36"/>
<connect gate="G$1" pin="IVDD@2" pad="79"/>
<connect gate="G$1" pin="IVDD@3" pad="97"/>
<connect gate="G$1" pin="IVDD@4" pad="125"/>
<connect gate="G$1" pin="IVDD@5" pad="156"/>
<connect gate="G$1" pin="JTAG_EN" pad="96"/>
<connect gate="G$1" pin="PLL_VDD" pad="99"/>
<connect gate="G$1" pin="PLL_VSS" pad="98"/>
<connect gate="G$1" pin="PSTCLK" pad="70"/>
<connect gate="G$1" pin="QSPI_CLK" pad="77"/>
<connect gate="G$1" pin="QSPI_CS2" pad="78"/>
<connect gate="G$1" pin="QSPI_DIN" pad="75"/>
<connect gate="G$1" pin="QSPI_DOUT" pad="76"/>
<connect gate="G$1" pin="R/!W" pad="65"/>
<connect gate="G$1" pin="SD_A10" pad="43"/>
<connect gate="G$1" pin="SD_CKE" pad="14"/>
<connect gate="G$1" pin="SD_CLK" pad="37"/>
<connect gate="G$1" pin="SD_DQS1/3" pad="25"/>
<connect gate="G$1" pin="SD_DQS2" pad="55"/>
<connect gate="G$1" pin="SD_SDR_DQS" pad="35"/>
<connect gate="G$1" pin="SD_VDD@1" pad="11"/>
<connect gate="G$1" pin="SD_VDD@2" pad="39"/>
<connect gate="G$1" pin="SD_VDD@3" pad="41"/>
<connect gate="G$1" pin="SD_VDD@4" pad="67"/>
<connect gate="G$1" pin="SD_VDD@5" pad="105"/>
<connect gate="G$1" pin="SD_VDD@6" pad="121"/>
<connect gate="G$1" pin="SD_VDD@7" pad="137"/>
<connect gate="G$1" pin="TEST" pad="124"/>
<connect gate="G$1" pin="TMS/!BKPT" pad="87"/>
<connect gate="G$1" pin="U0RXD" pad="80"/>
<connect gate="G$1" pin="U0TXD" pad="83"/>
<connect gate="G$1" pin="U1RXD" pad="140"/>
<connect gate="G$1" pin="U1TXD" pad="141"/>
<connect gate="G$1" pin="VSS@1" pad="10"/>
<connect gate="G$1" pin="VSS@2" pad="42"/>
<connect gate="G$1" pin="VSS@3" pad="68"/>
<connect gate="G$1" pin="VSS@4" pad="82"/>
<connect gate="G$1" pin="VSS@5" pad="89"/>
<connect gate="G$1" pin="VSS@6" pad="104"/>
<connect gate="G$1" pin="VSS@7" pad="122"/>
<connect gate="G$1" pin="VSS@8" pad="138"/>
<connect gate="G$1" pin="VSS@9" pad="159"/>
<connect gate="G$1" pin="XTAL2" pad="93"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCF53*" prefix="IC">
<description>&lt;b&gt;MCF537x ColdFire® Microprocessor&lt;/b&gt;&lt;p&gt;
Source: www.freescale.com .. MCF5373DS.pdf&lt;br&gt;</description>
<gates>
<gate name="A" symbol="MCF537X-CONTROL"/>
<gate name="B" symbol="MCF537X-FEC"/>
<gate name="C" symbol="MCF537X-FLEXBUS"/>
<gate name="D" symbol="MCF537X-IO"/>
<gate name="E" symbol="MCF537X-SDRAM"/>
<gate name="P" symbol="MCF537X-PWR"/>
</gates>
<devices>
<device name="" package="MAPGBA196">
<connects>
<connect gate="A" pin="!BKPT" pad="L13"/>
<connect gate="A" pin="!IRQ1" pad="G11"/>
<connect gate="A" pin="!IRQ2" pad="G12"/>
<connect gate="A" pin="!IRQ3" pad="G13"/>
<connect gate="A" pin="!IRQ4" pad="G14"/>
<connect gate="A" pin="!IRQ5" pad="F11"/>
<connect gate="A" pin="!IRQ6" pad="F12"/>
<connect gate="A" pin="!IRQ7" pad="F13"/>
<connect gate="A" pin="!RCON" pad="P8"/>
<connect gate="A" pin="!RESET" pad="K13"/>
<connect gate="A" pin="!RSTOUT" pad="L12"/>
<connect gate="A" pin="DDATA0" pad="P9"/>
<connect gate="A" pin="DDATA1" pad="N9"/>
<connect gate="A" pin="DDATA2" pad="M9"/>
<connect gate="A" pin="DDATA3" pad="L9,"/>
<connect gate="A" pin="DRAMSEL" pad="J11"/>
<connect gate="A" pin="DSCLK" pad="K11"/>
<connect gate="A" pin="DSI" pad="K12"/>
<connect gate="A" pin="DSO" pad="L11"/>
<connect gate="A" pin="DT0IN" pad="D3"/>
<connect gate="A" pin="DT1IN" pad="D2"/>
<connect gate="A" pin="DT2IN" pad="C1"/>
<connect gate="A" pin="DT3IN" pad="D1"/>
<connect gate="A" pin="EXTAL" pad="L14"/>
<connect gate="A" pin="EXTAL32K" pad="P13"/>
<connect gate="A" pin="FB_CLK" pad="N1"/>
<connect gate="A" pin="JTAG_EN" pad="G10"/>
<connect gate="A" pin="PST0" pad="P10"/>
<connect gate="A" pin="PST1" pad="N10"/>
<connect gate="A" pin="PST2" pad="M10"/>
<connect gate="A" pin="PST3" pad="L10"/>
<connect gate="A" pin="PSTCLK" pad="N8"/>
<connect gate="A" pin="TEST" pad="E10"/>
<connect gate="A" pin="XTAL" pad="K14"/>
<connect gate="A" pin="XTAL32K" pad="N13"/>
<connect gate="B" pin="FEC_COL" pad="B6"/>
<connect gate="B" pin="FEC_CRS" pad="A6"/>
<connect gate="B" pin="FEC_MDC" pad="B1"/>
<connect gate="B" pin="FEC_MDIO" pad="A1"/>
<connect gate="B" pin="FEC_RXCLK" pad="A5"/>
<connect gate="B" pin="FEC_RXD0" pad="B4"/>
<connect gate="B" pin="FEC_RXD1" pad="A4"/>
<connect gate="B" pin="FEC_RXD2" pad="D5"/>
<connect gate="B" pin="FEC_RXD3" pad="C5"/>
<connect gate="B" pin="FEC_RXDV" pad="B5"/>
<connect gate="B" pin="FEC_RXER" pad="C4"/>
<connect gate="B" pin="FEC_TXCLK" pad="A3"/>
<connect gate="B" pin="FEC_TXD0" pad="C2"/>
<connect gate="B" pin="FEC_TXD1" pad="B2"/>
<connect gate="B" pin="FEC_TXD2" pad="C3"/>
<connect gate="B" pin="FEC_TXD3" pad="D4"/>
<connect gate="B" pin="FEC_TXEN" pad="B3"/>
<connect gate="B" pin="FEC_TXER" pad="A2"/>
<connect gate="C" pin="!BE/BWE0" pad="P5"/>
<connect gate="C" pin="!BE/BWE1" pad="H2"/>
<connect gate="C" pin="!BE/BWE2" pad="M5"/>
<connect gate="C" pin="!BE/BWE3" pad="J3"/>
<connect gate="C" pin="!OE" pad="M8"/>
<connect gate="C" pin="!TA" pad="E14"/>
<connect gate="C" pin="!TS" pad="E2"/>
<connect gate="C" pin="A0" pad="D12"/>
<connect gate="C" pin="A1" pad="D13"/>
<connect gate="C" pin="A10" pad="A13"/>
<connect gate="C" pin="A11" pad="B12"/>
<connect gate="C" pin="A12" pad="A12"/>
<connect gate="C" pin="A13" pad="C11"/>
<connect gate="C" pin="A14" pad="B11"/>
<connect gate="C" pin="A15" pad="A11"/>
<connect gate="C" pin="A16" pad="D10"/>
<connect gate="C" pin="A17" pad="C10"/>
<connect gate="C" pin="A18" pad="B10"/>
<connect gate="C" pin="A19" pad="A10"/>
<connect gate="C" pin="A2" pad="D14"/>
<connect gate="C" pin="A20" pad="D9"/>
<connect gate="C" pin="A21" pad="C9"/>
<connect gate="C" pin="A22" pad="B9"/>
<connect gate="C" pin="A23" pad="A9"/>
<connect gate="C" pin="A3" pad="C13"/>
<connect gate="C" pin="A4" pad="C14"/>
<connect gate="C" pin="A5" pad="D11"/>
<connect gate="C" pin="A6" pad="C12"/>
<connect gate="C" pin="A7" pad="B13"/>
<connect gate="C" pin="A8" pad="B14"/>
<connect gate="C" pin="A9" pad="A14"/>
<connect gate="C" pin="D0" pad="P7"/>
<connect gate="C" pin="D1" pad="N7"/>
<connect gate="C" pin="D10" pad="G1"/>
<connect gate="C" pin="D11" pad="G2"/>
<connect gate="C" pin="D12" pad="G3"/>
<connect gate="C" pin="D13" pad="G4"/>
<connect gate="C" pin="D14" pad="F1"/>
<connect gate="C" pin="D15" pad="F2"/>
<connect gate="C" pin="D16" pad="P4"/>
<connect gate="C" pin="D17" pad="N4"/>
<connect gate="C" pin="D18" pad="P3"/>
<connect gate="C" pin="D19" pad="L5"/>
<connect gate="C" pin="D2" pad="M7"/>
<connect gate="C" pin="D20" pad="N3"/>
<connect gate="C" pin="D21" pad="P2"/>
<connect gate="C" pin="D22" pad="P1"/>
<connect gate="C" pin="D23" pad="N2"/>
<connect gate="C" pin="D24" pad="L3"/>
<connect gate="C" pin="D25" pad="L4"/>
<connect gate="C" pin="D26" pad="K1"/>
<connect gate="C" pin="D27" pad="K2"/>
<connect gate="C" pin="D28" pad="K3"/>
<connect gate="C" pin="D29" pad="K4"/>
<connect gate="C" pin="D3" pad="L7"/>
<connect gate="C" pin="D30" pad="J1"/>
<connect gate="C" pin="D31" pad="J2"/>
<connect gate="C" pin="D4" pad="P6"/>
<connect gate="C" pin="D5" pad="N6"/>
<connect gate="C" pin="D6" pad="M6"/>
<connect gate="C" pin="D7" pad="L6"/>
<connect gate="C" pin="D8" pad="H3"/>
<connect gate="C" pin="D9" pad="H4"/>
<connect gate="C" pin="R/!W" pad="L8"/>
<connect gate="D" pin="I2C_SCL2" pad="E3"/>
<connect gate="D" pin="I2C_SDA2" pad="E4"/>
<connect gate="D" pin="PWM1" pad="F14"/>
<connect gate="D" pin="PWM3" pad="E11"/>
<connect gate="D" pin="PWM5" pad="E12"/>
<connect gate="D" pin="PWM7" pad="E13"/>
<connect gate="D" pin="QSPI_CLK" pad="P12"/>
<connect gate="D" pin="QSPI_CS0" pad="M11"/>
<connect gate="D" pin="QSPI_CS1" pad="M12"/>
<connect gate="D" pin="QSPI_CS2" pad="N12"/>
<connect gate="D" pin="QSPI_DIN" pad="P11"/>
<connect gate="D" pin="QSPI_DOUT" pad="N11"/>
<connect gate="D" pin="U0CTS" pad="M14"/>
<connect gate="D" pin="U0RTS" pad="M13"/>
<connect gate="D" pin="U0RXD" pad="P14"/>
<connect gate="D" pin="U0TXD" pad="N14"/>
<connect gate="D" pin="U1CTS" pad="C6"/>
<connect gate="D" pin="U1RTS" pad="D6"/>
<connect gate="D" pin="U1RXD" pad="B7"/>
<connect gate="D" pin="U1TXD" pad="A7"/>
<connect gate="D" pin="USBHOST_M" pad="J13"/>
<connect gate="D" pin="USBHOST_P" pad="J12"/>
<connect gate="D" pin="USBOTG_M" pad="H14"/>
<connect gate="D" pin="USBOTG_P" pad="H13"/>
<connect gate="E" pin="!FB_CS0" pad="C7"/>
<connect gate="E" pin="!FB_CS1" pad="D7"/>
<connect gate="E" pin="!FB_CS2" pad="A8"/>
<connect gate="E" pin="!FB_CS3" pad="B8"/>
<connect gate="E" pin="!FB_CS4" pad="C8"/>
<connect gate="E" pin="!FB_CS5" pad="D8"/>
<connect gate="E" pin="!SD_CLK" pad="M1"/>
<connect gate="E" pin="!SD_CS0" pad="F3"/>
<connect gate="E" pin="!SD_SCAS" pad="M3"/>
<connect gate="E" pin="!SD_SRAS" pad="M4"/>
<connect gate="E" pin="!SD_WE" pad="E1"/>
<connect gate="E" pin="SD_A10" pad="M2"/>
<connect gate="E" pin="SD_CKE" pad="F4"/>
<connect gate="E" pin="SD_CLK" pad="L1"/>
<connect gate="E" pin="SD_DQS2" pad="N5"/>
<connect gate="E" pin="SD_DQS3" pad="H1"/>
<connect gate="E" pin="SD_SDR_DQS" pad="L2"/>
<connect gate="P" pin="EVDD@1" pad="E6"/>
<connect gate="P" pin="EVDD@10" pad="K9"/>
<connect gate="P" pin="EVDD@2" pad="E7"/>
<connect gate="P" pin="EVDD@3" pad="F5"/>
<connect gate="P" pin="EVDD@4" pad="F6"/>
<connect gate="P" pin="EVDD@5" pad="F7"/>
<connect gate="P" pin="EVDD@6" pad="G5"/>
<connect gate="P" pin="EVDD@7" pad="H10"/>
<connect gate="P" pin="EVDD@8" pad="J8"/>
<connect gate="P" pin="EVDD@9" pad="K8"/>
<connect gate="P" pin="IVDD@1" pad="E5"/>
<connect gate="P" pin="IVDD@2" pad="J9"/>
<connect gate="P" pin="IVDD@3" pad="K5"/>
<connect gate="P" pin="IVDD@4" pad="K10"/>
<connect gate="P" pin="PLL_VDD" pad="J10"/>
<connect gate="P" pin="PLL_VSS" pad="H11"/>
<connect gate="P" pin="SD_VDD@1" pad="E8"/>
<connect gate="P" pin="SD_VDD@10" pad="H5"/>
<connect gate="P" pin="SD_VDD@11" pad="K6"/>
<connect gate="P" pin="SD_VDD@12" pad="K7"/>
<connect gate="P" pin="SD_VDD@2" pad="E9"/>
<connect gate="P" pin="SD_VDD@3" pad="F8"/>
<connect gate="P" pin="SD_VDD@4" pad="F9"/>
<connect gate="P" pin="SD_VDD@5" pad="F10"/>
<connect gate="P" pin="SD_VDD@6" pad="J4"/>
<connect gate="P" pin="SD_VDD@7" pad="J5"/>
<connect gate="P" pin="SD_VDD@8" pad="J6"/>
<connect gate="P" pin="SD_VDD@9" pad="J7"/>
<connect gate="P" pin="USB_VDD" pad="H12"/>
<connect gate="P" pin="USB_VSS" pad="J14"/>
<connect gate="P" pin="VSS@1" pad="G6"/>
<connect gate="P" pin="VSS@2" pad="G7"/>
<connect gate="P" pin="VSS@3" pad="G8"/>
<connect gate="P" pin="VSS@4" pad="G9"/>
<connect gate="P" pin="VSS@5" pad="H6"/>
<connect gate="P" pin="VSS@6" pad="H7"/>
<connect gate="P" pin="VSS@7" pad="H8"/>
<connect gate="P" pin="VSS@8" pad="H9"/>
</connects>
<technologies>
<technology name="271">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="72L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCF5372LCVM240J"/>
<attribute name="OC_FARNELL" value="1380411"/>
<attribute name="OC_NEWARK" value="57R6122"/>
</technology>
<technology name="73L">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCF5373LCVM240J"/>
<attribute name="OC_FARNELL" value="1579871"/>
<attribute name="OC_NEWARK" value="57R6123"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S12XF-144" prefix="IC">
<description>&lt;b&gt;MC9S12XF512&lt;/b&gt;&lt;p&gt;
Source: www.freescale.com .. MC9S12XF512V1RM.pdf</description>
<gates>
<gate name="G$1" symbol="MC9S12XF-144"/>
</gates>
<devices>
<device name="" package="SQFP-S-20X20-144">
<connects>
<connect gate="G$1" pin="BKGD-MODC" pad="39"/>
<connect gate="G$1" pin="EXTAL" pad="58"/>
<connect gate="G$1" pin="NC" pad="56"/>
<connect gate="G$1" pin="NC@1" pad="111"/>
<connect gate="G$1" pin="NC@2" pad="112"/>
<connect gate="G$1" pin="NC@3" pad="121"/>
<connect gate="G$1" pin="NC@4" pad="122"/>
<connect gate="G$1" pin="NC@5" pad="129"/>
<connect gate="G$1" pin="NC@6" pad="130"/>
<connect gate="G$1" pin="PA0-ADDR8" pad="65"/>
<connect gate="G$1" pin="PA1-ADDR9" pad="66"/>
<connect gate="G$1" pin="PA2-ADDR10" pad="67"/>
<connect gate="G$1" pin="PA3-ADDR11" pad="68"/>
<connect gate="G$1" pin="PA4-ADDR12" pad="85"/>
<connect gate="G$1" pin="PA5-ADDR13" pad="86"/>
<connect gate="G$1" pin="PA6-ADDR14" pad="87"/>
<connect gate="G$1" pin="PA7-ADDR15" pad="88"/>
<connect gate="G$1" pin="PAD00-AN0" pad="91"/>
<connect gate="G$1" pin="PAD01-AN1" pad="93"/>
<connect gate="G$1" pin="PAD02-AN2" pad="95"/>
<connect gate="G$1" pin="PAD03-AN3" pad="97"/>
<connect gate="G$1" pin="PAD04-AN4" pad="99"/>
<connect gate="G$1" pin="PAD05-AN5" pad="101"/>
<connect gate="G$1" pin="PAD06-AN6" pad="103"/>
<connect gate="G$1" pin="PAD07-AN7" pad="105"/>
<connect gate="G$1" pin="PAD08-AN8" pad="92"/>
<connect gate="G$1" pin="PAD09-AN9" pad="94"/>
<connect gate="G$1" pin="PAD10-AN10" pad="96"/>
<connect gate="G$1" pin="PAD11-AN11" pad="98"/>
<connect gate="G$1" pin="PAD12-AN12" pad="100"/>
<connect gate="G$1" pin="PAD13-AN13" pad="102"/>
<connect gate="G$1" pin="PAD14-AN14" pad="104"/>
<connect gate="G$1" pin="PAD15-AN15" pad="106"/>
<connect gate="G$1" pin="PB0-ADDR0" pad="35"/>
<connect gate="G$1" pin="PB1-ADDR1" pad="36"/>
<connect gate="G$1" pin="PB2-ADDR2" pad="37"/>
<connect gate="G$1" pin="PB3-ADDR3" pad="38"/>
<connect gate="G$1" pin="PB4-ADDR4" pad="61"/>
<connect gate="G$1" pin="PB5-ADDR5" pad="62"/>
<connect gate="G$1" pin="PB6-ADDR6" pad="63"/>
<connect gate="G$1" pin="PB7-ADDR7" pad="64"/>
<connect gate="G$1" pin="PC0-DATA8" pad="22"/>
<connect gate="G$1" pin="PC1-DATA9" pad="23"/>
<connect gate="G$1" pin="PC2-DATA10" pad="24"/>
<connect gate="G$1" pin="PC3-DATA11" pad="25"/>
<connect gate="G$1" pin="PC4-DATA12" pad="26"/>
<connect gate="G$1" pin="PC5-DATA13" pad="27"/>
<connect gate="G$1" pin="PC6-DATA14" pad="28"/>
<connect gate="G$1" pin="PC7-DATA15" pad="29"/>
<connect gate="G$1" pin="PD0-DATA0" pad="6"/>
<connect gate="G$1" pin="PD1-DATA1" pad="5"/>
<connect gate="G$1" pin="PD2-DATA2" pad="4"/>
<connect gate="G$1" pin="PD3-DATA3" pad="3"/>
<connect gate="G$1" pin="PD4-DATA4" pad="138"/>
<connect gate="G$1" pin="PD5-DATA5" pad="137"/>
<connect gate="G$1" pin="PD6-DATA6" pad="136"/>
<connect gate="G$1" pin="PD7-DATA7" pad="135"/>
<connect gate="G$1" pin="PE0-XIRQ" pad="72"/>
<connect gate="G$1" pin="PE1-IRQ" pad="71"/>
<connect gate="G$1" pin="PE2-RW" pad="45"/>
<connect gate="G$1" pin="PE3-LSTRB" pad="44"/>
<connect gate="G$1" pin="PE4-ECLK" pad="43"/>
<connect gate="G$1" pin="PE5-MODA" pad="42"/>
<connect gate="G$1" pin="PE6-MODB" pad="41"/>
<connect gate="G$1" pin="PE7-XCLKS" pad="40"/>
<connect gate="G$1" pin="PH0-RXD_A" pad="73"/>
<connect gate="G$1" pin="PH1-TXD_A" pad="74"/>
<connect gate="G$1" pin="PH2-TXE_A" pad="75"/>
<connect gate="G$1" pin="PH3" pad="76"/>
<connect gate="G$1" pin="PH4-RXD_B" pad="46"/>
<connect gate="G$1" pin="PH5-TXD_B" pad="47"/>
<connect gate="G$1" pin="PH6-TXE_B" pad="48"/>
<connect gate="G$1" pin="PH7" pad="49"/>
<connect gate="G$1" pin="PJ0-IS0" pad="11"/>
<connect gate="G$1" pin="PJ1-IS1" pad="12"/>
<connect gate="G$1" pin="PJ2-IS2" pad="13"/>
<connect gate="G$1" pin="PJ3-STB0" pad="30"/>
<connect gate="G$1" pin="PJ4-STB1" pad="31"/>
<connect gate="G$1" pin="PJ5-STB2" pad="32"/>
<connect gate="G$1" pin="PJ6-STB3" pad="33"/>
<connect gate="G$1" pin="PJ7" pad="34"/>
<connect gate="G$1" pin="PK0-ADDR16" pad="77"/>
<connect gate="G$1" pin="PK1-ADDR17" pad="78"/>
<connect gate="G$1" pin="PK2-ADDR18" pad="79"/>
<connect gate="G$1" pin="PK3-ADDR19" pad="80"/>
<connect gate="G$1" pin="PK4-ADDR20" pad="81"/>
<connect gate="G$1" pin="PK5-ADDR21" pad="82"/>
<connect gate="G$1" pin="PK6-ADDR22" pad="83"/>
<connect gate="G$1" pin="PK7-EWAIT" pad="84"/>
<connect gate="G$1" pin="PM0-RXCAN0" pad="132"/>
<connect gate="G$1" pin="PM1-TXCAN0" pad="131"/>
<connect gate="G$1" pin="PM2-FAULT2" pad="128"/>
<connect gate="G$1" pin="PM3-FAULT3" pad="127"/>
<connect gate="G$1" pin="PM4-MISO1" pad="126"/>
<connect gate="G$1" pin="PM5-MOSI1" pad="125"/>
<connect gate="G$1" pin="PM6-SCK1" pad="124"/>
<connect gate="G$1" pin="PM7-SS1" pad="123"/>
<connect gate="G$1" pin="PP0-PMF0" pad="2"/>
<connect gate="G$1" pin="PP1-PMF1" pad="1"/>
<connect gate="G$1" pin="PP2-PMF2" pad="144"/>
<connect gate="G$1" pin="PP3-PMF3" pad="143"/>
<connect gate="G$1" pin="PP4-PMF4" pad="142"/>
<connect gate="G$1" pin="PP5-PMF5" pad="141"/>
<connect gate="G$1" pin="PP6-FAULT0" pad="140"/>
<connect gate="G$1" pin="PP7-FAULT1" pad="139"/>
<connect gate="G$1" pin="PS0-RXD0" pad="113"/>
<connect gate="G$1" pin="PS1-TXD0" pad="114"/>
<connect gate="G$1" pin="PS2-RXD1" pad="115"/>
<connect gate="G$1" pin="PS3-TXD1" pad="116"/>
<connect gate="G$1" pin="PS4-MISO0" pad="117"/>
<connect gate="G$1" pin="PS5-MOSI0" pad="118"/>
<connect gate="G$1" pin="PS6-SCK0" pad="119"/>
<connect gate="G$1" pin="PS7-SS0" pad="120"/>
<connect gate="G$1" pin="PT0-IOC0" pad="7"/>
<connect gate="G$1" pin="PT1-IOC1" pad="8"/>
<connect gate="G$1" pin="PT2-IOC2" pad="9"/>
<connect gate="G$1" pin="PT3-IOC3" pad="10"/>
<connect gate="G$1" pin="PT4-IOC4" pad="18"/>
<connect gate="G$1" pin="PT5-IOC5" pad="19"/>
<connect gate="G$1" pin="PT6-IOC6" pad="20"/>
<connect gate="G$1" pin="PT7-IOC7" pad="21"/>
<connect gate="G$1" pin="RESET" pad="54"/>
<connect gate="G$1" pin="TEST" pad="60"/>
<connect gate="G$1" pin="VDD@1" pad="89"/>
<connect gate="G$1" pin="VDDA" pad="107"/>
<connect gate="G$1" pin="VDDF" pad="14"/>
<connect gate="G$1" pin="VDDPLL" pad="55"/>
<connect gate="G$1" pin="VDDR" pad="53"/>
<connect gate="G$1" pin="VDDX@1" pad="134"/>
<connect gate="G$1" pin="VDDX@2" pad="50"/>
<connect gate="G$1" pin="VDDX@3" pad="17"/>
<connect gate="G$1" pin="VDDX@4" pad="69"/>
<connect gate="G$1" pin="VRH" pad="108"/>
<connect gate="G$1" pin="VRL" pad="109"/>
<connect gate="G$1" pin="VSS@1" pad="15"/>
<connect gate="G$1" pin="VSS@3" pad="52"/>
<connect gate="G$1" pin="VSSA" pad="110"/>
<connect gate="G$1" pin="VSSPLL" pad="57"/>
<connect gate="G$1" pin="VSSQ2" pad="90"/>
<connect gate="G$1" pin="VSSX@1" pad="133"/>
<connect gate="G$1" pin="VSSX@2" pad="51"/>
<connect gate="G$1" pin="VSSX@3" pad="16"/>
<connect gate="G$1" pin="VSSX@4" pad="70"/>
<connect gate="G$1" pin="XTAL" pad="59"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LFDAS12XFLT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="14M5920"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S12XF-112" prefix="IC">
<description>&lt;b&gt;MC9S12XF512&lt;/b&gt;&lt;p&gt;
Source: www.freescale.com .. MC9S12XF512V1RM.pdf</description>
<gates>
<gate name="G$1" symbol="MC9S12XF-112"/>
</gates>
<devices>
<device name="" package="SQFP-S-20X20-112">
<connects>
<connect gate="G$1" pin="BKGD-MODC" pad="29"/>
<connect gate="G$1" pin="EXTAL" pad="48"/>
<connect gate="G$1" pin="NC" pad="46"/>
<connect gate="G$1" pin="PA0-ADDR8" pad="51"/>
<connect gate="G$1" pin="PA1-ADDR9" pad="52"/>
<connect gate="G$1" pin="PA2-ADDR10" pad="53"/>
<connect gate="G$1" pin="PA3-ADDR11" pad="54"/>
<connect gate="G$1" pin="PA4-ADDR12" pad="61"/>
<connect gate="G$1" pin="PA5-ADDR13" pad="62"/>
<connect gate="G$1" pin="PA6-ADDR14" pad="63"/>
<connect gate="G$1" pin="PA7-ADDR15" pad="64"/>
<connect gate="G$1" pin="PAD00-AN0" pad="67"/>
<connect gate="G$1" pin="PAD01-AN1" pad="69"/>
<connect gate="G$1" pin="PAD02-AN2" pad="71"/>
<connect gate="G$1" pin="PAD03-AN3" pad="73"/>
<connect gate="G$1" pin="PAD04-AN4" pad="75"/>
<connect gate="G$1" pin="PAD05-AN5" pad="77"/>
<connect gate="G$1" pin="PAD06-AN6" pad="79"/>
<connect gate="G$1" pin="PAD07-AN7" pad="81"/>
<connect gate="G$1" pin="PAD08-AN8" pad="68"/>
<connect gate="G$1" pin="PAD09-AN9" pad="70"/>
<connect gate="G$1" pin="PAD10-AN10" pad="72"/>
<connect gate="G$1" pin="PAD11-AN11" pad="74"/>
<connect gate="G$1" pin="PAD12-AN12" pad="76"/>
<connect gate="G$1" pin="PAD13-AN13" pad="78"/>
<connect gate="G$1" pin="PAD14-AN14" pad="80"/>
<connect gate="G$1" pin="PAD15-AN15" pad="82"/>
<connect gate="G$1" pin="PB0-ADDR0" pad="27"/>
<connect gate="G$1" pin="PB1-ADDR1" pad="28"/>
<connect gate="G$1" pin="PD0-DATA0" pad="6"/>
<connect gate="G$1" pin="PD1-DATA1" pad="5"/>
<connect gate="G$1" pin="PD2-DATA2" pad="4"/>
<connect gate="G$1" pin="PD3-DATA3" pad="3"/>
<connect gate="G$1" pin="PD4-DATA4" pad="106"/>
<connect gate="G$1" pin="PD5-DATA5" pad="105"/>
<connect gate="G$1" pin="PE0-XIRQ" pad="56"/>
<connect gate="G$1" pin="PE1-IRQ" pad="55"/>
<connect gate="G$1" pin="PE2-RW" pad="35"/>
<connect gate="G$1" pin="PE3-LSTRB" pad="34"/>
<connect gate="G$1" pin="PE4-ECLK" pad="33"/>
<connect gate="G$1" pin="PE5-MODA" pad="32"/>
<connect gate="G$1" pin="PE6-MODB" pad="31"/>
<connect gate="G$1" pin="PE7-XCLKS" pad="30"/>
<connect gate="G$1" pin="PH0-RXD_A" pad="57"/>
<connect gate="G$1" pin="PH1-TXD_A" pad="58"/>
<connect gate="G$1" pin="PH2-TXE_A" pad="59"/>
<connect gate="G$1" pin="PH3" pad="60"/>
<connect gate="G$1" pin="PH4-RXD_B" pad="36"/>
<connect gate="G$1" pin="PH5-TXD_B" pad="37"/>
<connect gate="G$1" pin="PH6-TXE_B" pad="38"/>
<connect gate="G$1" pin="PH7" pad="39"/>
<connect gate="G$1" pin="PJ0-IS0" pad="11"/>
<connect gate="G$1" pin="PJ1-IS1" pad="12"/>
<connect gate="G$1" pin="PJ2-IS2" pad="13"/>
<connect gate="G$1" pin="PJ3-STB0" pad="22"/>
<connect gate="G$1" pin="PJ4-STB1" pad="23"/>
<connect gate="G$1" pin="PJ5-STB2" pad="24"/>
<connect gate="G$1" pin="PJ6-STB3" pad="25"/>
<connect gate="G$1" pin="PJ7" pad="26"/>
<connect gate="G$1" pin="PM0-RXCAN0" pad="102"/>
<connect gate="G$1" pin="PM1-TXCAN0" pad="101"/>
<connect gate="G$1" pin="PM2-FAULT2" pad="100"/>
<connect gate="G$1" pin="PM3-FAULT3" pad="99"/>
<connect gate="G$1" pin="PM4-MISO1" pad="98"/>
<connect gate="G$1" pin="PM5-MOSI1" pad="97"/>
<connect gate="G$1" pin="PM6-SCK1" pad="96"/>
<connect gate="G$1" pin="PM7-SS1" pad="95"/>
<connect gate="G$1" pin="PP0-PMF0" pad="2"/>
<connect gate="G$1" pin="PP1-PMF1" pad="1"/>
<connect gate="G$1" pin="PP2-PMF2" pad="112"/>
<connect gate="G$1" pin="PP3-PMF3" pad="111"/>
<connect gate="G$1" pin="PP4-PMF4" pad="110"/>
<connect gate="G$1" pin="PP5-PMF5" pad="109"/>
<connect gate="G$1" pin="PP6-FAULT0" pad="108"/>
<connect gate="G$1" pin="PP7-FAULT1" pad="107"/>
<connect gate="G$1" pin="PS0-RXD0" pad="87"/>
<connect gate="G$1" pin="PS1-TXD0" pad="88"/>
<connect gate="G$1" pin="PS2-RXD1" pad="89"/>
<connect gate="G$1" pin="PS3-TXD1" pad="90"/>
<connect gate="G$1" pin="PS4-MISO0" pad="91"/>
<connect gate="G$1" pin="PS5-MOSI0" pad="92"/>
<connect gate="G$1" pin="PS6-SCK0" pad="93"/>
<connect gate="G$1" pin="PS7-SS0" pad="94"/>
<connect gate="G$1" pin="PT0-IOC0" pad="7"/>
<connect gate="G$1" pin="PT1-IOC1" pad="8"/>
<connect gate="G$1" pin="PT2-IOC2" pad="9"/>
<connect gate="G$1" pin="PT3-IOC3" pad="10"/>
<connect gate="G$1" pin="PT4-IOC4" pad="18"/>
<connect gate="G$1" pin="PT5-IOC5" pad="19"/>
<connect gate="G$1" pin="PT6-IOC6" pad="20"/>
<connect gate="G$1" pin="PT7-IOC7" pad="21"/>
<connect gate="G$1" pin="RESET" pad="44"/>
<connect gate="G$1" pin="TEST" pad="50"/>
<connect gate="G$1" pin="VDD@1" pad="65"/>
<connect gate="G$1" pin="VDDA" pad="83"/>
<connect gate="G$1" pin="VDDF5" pad="14"/>
<connect gate="G$1" pin="VDDPLL" pad="45"/>
<connect gate="G$1" pin="VDDR" pad="43"/>
<connect gate="G$1" pin="VDDX@1" pad="104"/>
<connect gate="G$1" pin="VDDX@2" pad="40"/>
<connect gate="G$1" pin="VDDX@3" pad="17"/>
<connect gate="G$1" pin="VRH" pad="84"/>
<connect gate="G$1" pin="VRL" pad="85"/>
<connect gate="G$1" pin="VSS@1" pad="15"/>
<connect gate="G$1" pin="VSS@2" pad="66"/>
<connect gate="G$1" pin="VSS@3" pad="42"/>
<connect gate="G$1" pin="VSSA" pad="86"/>
<connect gate="G$1" pin="VSSPLL" pad="47"/>
<connect gate="G$1" pin="VSSX@1" pad="103"/>
<connect gate="G$1" pin="VSSX@2" pad="41"/>
<connect gate="G$1" pin="VSSX@3" pad="16"/>
<connect gate="G$1" pin="XTAL" pad="49"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S12XF-64" prefix="IC">
<description>&lt;b&gt;MC9S12XF512&lt;/b&gt;&lt;p&gt;
Source: www.freescale.com .. MC9S12XF512V1RM.pdf</description>
<gates>
<gate name="G$1" symbol="MC9S12XF-64"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="BKGD-MODC" pad="17"/>
<connect gate="G$1" pin="EXTAL" pad="28"/>
<connect gate="G$1" pin="NC" pad="26"/>
<connect gate="G$1" pin="PAD00-AN0" pad="39"/>
<connect gate="G$1" pin="PAD01-AN1" pad="40"/>
<connect gate="G$1" pin="PAD02-AN2" pad="41"/>
<connect gate="G$1" pin="PAD03-AN3" pad="42"/>
<connect gate="G$1" pin="PAD04-AN4" pad="43"/>
<connect gate="G$1" pin="PAD05-AN5" pad="44"/>
<connect gate="G$1" pin="PAD06-AN6" pad="45"/>
<connect gate="G$1" pin="PAD07-AN7" pad="46"/>
<connect gate="G$1" pin="PE0-XIRQ" pad="32"/>
<connect gate="G$1" pin="PE1-IRQ" pad="31"/>
<connect gate="G$1" pin="PE4-ECLK" pad="19"/>
<connect gate="G$1" pin="PE7-XCLKS" pad="18"/>
<connect gate="G$1" pin="PH0-RXD_A" pad="33"/>
<connect gate="G$1" pin="PH1-TXD_A" pad="34"/>
<connect gate="G$1" pin="PH2-TXE_A" pad="35"/>
<connect gate="G$1" pin="PH3" pad="36"/>
<connect gate="G$1" pin="PJ3-STB0" pad="13"/>
<connect gate="G$1" pin="PJ4-STB1" pad="14"/>
<connect gate="G$1" pin="PJ5-STB2" pad="15"/>
<connect gate="G$1" pin="PJ6-STB3" pad="16"/>
<connect gate="G$1" pin="PM0-RXCAN0" pad="58"/>
<connect gate="G$1" pin="PM1-TXCAN0" pad="57"/>
<connect gate="G$1" pin="PP0-PMF0" pad="2"/>
<connect gate="G$1" pin="PP1-PMF1" pad="1"/>
<connect gate="G$1" pin="PP2-PMF2" pad="64"/>
<connect gate="G$1" pin="PP3-PMF3" pad="63"/>
<connect gate="G$1" pin="PP4-PMF4" pad="62"/>
<connect gate="G$1" pin="PP5-PMF5" pad="61"/>
<connect gate="G$1" pin="PS0-RXD0" pad="51"/>
<connect gate="G$1" pin="PS1-TXD0" pad="52"/>
<connect gate="G$1" pin="PS4-MISO0" pad="53"/>
<connect gate="G$1" pin="PS5-MOSI0" pad="54"/>
<connect gate="G$1" pin="PS6-SCK0" pad="55"/>
<connect gate="G$1" pin="PS7-SS0" pad="56"/>
<connect gate="G$1" pin="PT0-IOC0" pad="3"/>
<connect gate="G$1" pin="PT1-IOC1" pad="4"/>
<connect gate="G$1" pin="PT2-IOC2" pad="5"/>
<connect gate="G$1" pin="PT3-IOC3" pad="6"/>
<connect gate="G$1" pin="PT4-IOC4" pad="9"/>
<connect gate="G$1" pin="PT5-IOC5" pad="10"/>
<connect gate="G$1" pin="PT6-IOC6" pad="11"/>
<connect gate="G$1" pin="PT7-IOC7" pad="12"/>
<connect gate="G$1" pin="RESET" pad="24"/>
<connect gate="G$1" pin="TEST" pad="30"/>
<connect gate="G$1" pin="VDD@1" pad="37"/>
<connect gate="G$1" pin="VDDA" pad="47"/>
<connect gate="G$1" pin="VDDF5" pad="7"/>
<connect gate="G$1" pin="VDDPLL" pad="25"/>
<connect gate="G$1" pin="VDDR" pad="23"/>
<connect gate="G$1" pin="VDDX2" pad="20"/>
<connect gate="G$1" pin="VDDX@1" pad="60"/>
<connect gate="G$1" pin="VRH" pad="48"/>
<connect gate="G$1" pin="VRL" pad="49"/>
<connect gate="G$1" pin="VSS@1" pad="8"/>
<connect gate="G$1" pin="VSS@2" pad="38"/>
<connect gate="G$1" pin="VSS@3" pad="22"/>
<connect gate="G$1" pin="VSSA" pad="50"/>
<connect gate="G$1" pin="VSSPLL" pad="27"/>
<connect gate="G$1" pin="VSSX2" pad="21"/>
<connect gate="G$1" pin="VSSX@1" pad="59"/>
<connect gate="G$1" pin="XTAL" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33932" prefix="IC">
<description>&lt;b&gt;5.0 A Throttle Control H-Bridge&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://www.freescale.com/files/analog/doc/data_sheet/MC33932.pdf?fpsp=1</description>
<gates>
<gate name="G$1" symbol="MC33932"/>
</gates>
<devices>
<device name="" package="HSOP44">
<connects>
<connect gate="G$1" pin="!SFA" pad="44"/>
<connect gate="G$1" pin="!SFB" pad="22"/>
<connect gate="G$1" pin="CCPA" pad="41"/>
<connect gate="G$1" pin="CCPB" pad="19"/>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D3" pad="23"/>
<connect gate="G$1" pin="EH@1" pad="EH@1"/>
<connect gate="G$1" pin="EH@2" pad="EH@2"/>
<connect gate="G$1" pin="EH@3" pad="EH@3"/>
<connect gate="G$1" pin="EN/!D2" pad="3"/>
<connect gate="G$1" pin="EN/!D4" pad="25"/>
<connect gate="G$1" pin="FBA" pad="2"/>
<connect gate="G$1" pin="FBB" pad="24"/>
<connect gate="G$1" pin="IN1" pad="43"/>
<connect gate="G$1" pin="IN2" pad="42"/>
<connect gate="G$1" pin="IN3" pad="21"/>
<connect gate="G$1" pin="IN4" pad="20"/>
<connect gate="G$1" pin="OUT1" pad="7"/>
<connect gate="G$1" pin="OUT1@1" pad="8"/>
<connect gate="G$1" pin="OUT1@2" pad="9"/>
<connect gate="G$1" pin="OUT2" pad="36"/>
<connect gate="G$1" pin="OUT2@1" pad="37"/>
<connect gate="G$1" pin="OUT2@2" pad="38"/>
<connect gate="G$1" pin="OUT3" pad="29"/>
<connect gate="G$1" pin="OUT3@1" pad="30"/>
<connect gate="G$1" pin="OUT3@2" pad="31"/>
<connect gate="G$1" pin="OUT4" pad="14"/>
<connect gate="G$1" pin="OUT4@1" pad="15"/>
<connect gate="G$1" pin="OUT4@2" pad="16"/>
<connect gate="G$1" pin="PGNDA" pad="10"/>
<connect gate="G$1" pin="PGNDA@1" pad="11"/>
<connect gate="G$1" pin="PGNDA@2" pad="34"/>
<connect gate="G$1" pin="PGNDA@3" pad="35"/>
<connect gate="G$1" pin="PGNDB" pad="12"/>
<connect gate="G$1" pin="PGNDB@1" pad="13"/>
<connect gate="G$1" pin="PGNDB@2" pad="32"/>
<connect gate="G$1" pin="PGNDB@3" pad="33"/>
<connect gate="G$1" pin="VPWRA" pad="4"/>
<connect gate="G$1" pin="VPWRA@1" pad="5"/>
<connect gate="G$1" pin="VPWRA@2" pad="6"/>
<connect gate="G$1" pin="VPWRA@3" pad="39"/>
<connect gate="G$1" pin="VPWRA@4" pad="40"/>
<connect gate="G$1" pin="VPWRB" pad="17"/>
<connect gate="G$1" pin="VPWRB@1" pad="18"/>
<connect gate="G$1" pin="VPWRB@2" pad="26"/>
<connect gate="G$1" pin="VPWRB@3" pad="27"/>
<connect gate="G$1" pin="VPWRB@4" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC33932VW"/>
<attribute name="OC_FARNELL" value="1701639"/>
<attribute name="OC_NEWARK" value="67P3304"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S08GT*A-48" prefix="IC">
<description>&lt;b&gt;HCS08 Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC9S08GT16A.pdf</description>
<gates>
<gate name="G$1" symbol="MC9S08GT16A"/>
</gates>
<devices>
<device name="" package="QFN48">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="IRQ" pad="12"/>
<connect gate="G$1" pin="PTA0/KBIP0" pad="35"/>
<connect gate="G$1" pin="PTA1/KBIP1" pad="36"/>
<connect gate="G$1" pin="PTA2/KBIP2" pad="37"/>
<connect gate="G$1" pin="PTA3/KBIP3" pad="38"/>
<connect gate="G$1" pin="PTA4/KBIP4" pad="39"/>
<connect gate="G$1" pin="PTA5/KBIP5" pad="40"/>
<connect gate="G$1" pin="PTA6/KBIP6" pad="41"/>
<connect gate="G$1" pin="PTA7/KBIP7" pad="42"/>
<connect gate="G$1" pin="PTB0/ADP0" pad="25"/>
<connect gate="G$1" pin="PTB1/ADP1" pad="26"/>
<connect gate="G$1" pin="PTB2/ADP2" pad="27"/>
<connect gate="G$1" pin="PTB3/ADP3" pad="28"/>
<connect gate="G$1" pin="PTB4/ADP4" pad="29"/>
<connect gate="G$1" pin="PTB5/ADP5" pad="30"/>
<connect gate="G$1" pin="PTB6/ADP6" pad="31"/>
<connect gate="G$1" pin="PTB7/ADP7" pad="32"/>
<connect gate="G$1" pin="PTC0/TXD2" pad="2"/>
<connect gate="G$1" pin="PTC1/RXD2" pad="3"/>
<connect gate="G$1" pin="PTC2/SDA" pad="4"/>
<connect gate="G$1" pin="PTC3/SCL" pad="5"/>
<connect gate="G$1" pin="PTC4" pad="6"/>
<connect gate="G$1" pin="PTC5" pad="7"/>
<connect gate="G$1" pin="PTC6" pad="8"/>
<connect gate="G$1" pin="PTC7" pad="9"/>
<connect gate="G$1" pin="PTD0/TPM1CLK/TPM1CH0" pad="20"/>
<connect gate="G$1" pin="PTD1/TPM1CH1" pad="21"/>
<connect gate="G$1" pin="PTD2/TPM1CH2" pad="22"/>
<connect gate="G$1" pin="PTD3/TPM2CLK/TPM2CH0" pad="23"/>
<connect gate="G$1" pin="PTD4/TPM2CH1" pad="24"/>
<connect gate="G$1" pin="PTE0/TXD1" pad="10"/>
<connect gate="G$1" pin="PTE1/RXD1" pad="11"/>
<connect gate="G$1" pin="PTE2/!SS" pad="13"/>
<connect gate="G$1" pin="PTE3/MISO" pad="14"/>
<connect gate="G$1" pin="PTE4/MOSI" pad="15"/>
<connect gate="G$1" pin="PTE5/SPSCK" pad="16"/>
<connect gate="G$1" pin="PTG0/BKGD/MS" pad="45"/>
<connect gate="G$1" pin="PTG1/XTAL" pad="46"/>
<connect gate="G$1" pin="PTG2/EXTAL" pad="47"/>
<connect gate="G$1" pin="PTG3" pad="48"/>
<connect gate="G$1" pin="VDD" pad="19"/>
<connect gate="G$1" pin="VDDAD" pad="43"/>
<connect gate="G$1" pin="VREFH" pad="33"/>
<connect gate="G$1" pin="VREFL" pad="34"/>
<connect gate="G$1" pin="VSS@1" pad="17"/>
<connect gate="G$1" pin="VSS@2" pad="18"/>
<connect gate="G$1" pin="VSSAD" pad="44"/>
</connects>
<technologies>
<technology name="16">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC9S08GT16ACFDE"/>
<attribute name="OC_FARNELL" value="1579705"/>
<attribute name="OC_NEWARK" value="01M5861"/>
</technology>
<technology name="8">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC9S08GT8AMFDE"/>
<attribute name="OC_FARNELL" value="1294360"/>
<attribute name="OC_NEWARK" value="01M5874"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S08GT*A-44" prefix="IC">
<description>&lt;b&gt;HCS08 Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC9S08GT16A.pdf</description>
<gates>
<gate name="G$1" symbol="MC9S08GT16A-44"/>
</gates>
<devices>
<device name="" package="QFP44">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="IRQ" pad="11"/>
<connect gate="G$1" pin="PTA0/KBIP0" pad="32"/>
<connect gate="G$1" pin="PTA1/KBIP1" pad="33"/>
<connect gate="G$1" pin="PTA2/KBIP2" pad="34"/>
<connect gate="G$1" pin="PTA3/KBIP3" pad="35"/>
<connect gate="G$1" pin="PTA4/KBIP4" pad="36"/>
<connect gate="G$1" pin="PTA5/KBIP5" pad="37"/>
<connect gate="G$1" pin="PTA6/KBIP6" pad="38"/>
<connect gate="G$1" pin="PTA7/KBIP7" pad="39"/>
<connect gate="G$1" pin="PTB0/ADP0" pad="22"/>
<connect gate="G$1" pin="PTB1/ADP1" pad="23"/>
<connect gate="G$1" pin="PTB2/ADP2" pad="24"/>
<connect gate="G$1" pin="PTB3/ADP3" pad="25"/>
<connect gate="G$1" pin="PTB4/ADP4" pad="26"/>
<connect gate="G$1" pin="PTB5/ADP5" pad="27"/>
<connect gate="G$1" pin="PTB6/ADP6" pad="28"/>
<connect gate="G$1" pin="PTB7/ADP7" pad="29"/>
<connect gate="G$1" pin="PTC0/TXD2" pad="2"/>
<connect gate="G$1" pin="PTC1/RXD2" pad="3"/>
<connect gate="G$1" pin="PTC2/SDA" pad="4"/>
<connect gate="G$1" pin="PTC3/SCL" pad="5"/>
<connect gate="G$1" pin="PTC4" pad="6"/>
<connect gate="G$1" pin="PTC5" pad="7"/>
<connect gate="G$1" pin="PTC6" pad="8"/>
<connect gate="G$1" pin="PTD0/TPM1CLK/TPM1CH0" pad="18"/>
<connect gate="G$1" pin="PTD1/TPM1CH1" pad="19"/>
<connect gate="G$1" pin="PTD3/TPM2CLK/TPM2CH0" pad="20"/>
<connect gate="G$1" pin="PTD4/TPM2CH1" pad="21"/>
<connect gate="G$1" pin="PTE0/TXD1" pad="9"/>
<connect gate="G$1" pin="PTE1/RXD1" pad="10"/>
<connect gate="G$1" pin="PTE2/!SS" pad="12"/>
<connect gate="G$1" pin="PTE3/MISO" pad="13"/>
<connect gate="G$1" pin="PTE4/MOSI" pad="14"/>
<connect gate="G$1" pin="PTE5/SPSCK" pad="15"/>
<connect gate="G$1" pin="PTG0/BKGD/MS" pad="42"/>
<connect gate="G$1" pin="PTG1/XTAL" pad="43"/>
<connect gate="G$1" pin="PTG2/EXTAL" pad="44"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VDDAD" pad="40"/>
<connect gate="G$1" pin="VREFH" pad="30"/>
<connect gate="G$1" pin="VREFL" pad="31"/>
<connect gate="G$1" pin="VSS@1" pad="16"/>
<connect gate="G$1" pin="VSSAD" pad="41"/>
</connects>
<technologies>
<technology name="16">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC9S08GT16ACFBE"/>
<attribute name="OC_FARNELL" value="1579706"/>
<attribute name="OC_NEWARK" value="01M5859"/>
</technology>
<technology name="8">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC9S08GT8AMFBE"/>
<attribute name="OC_FARNELL" value="1294361"/>
<attribute name="OC_NEWARK" value="01M5872"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S08GT*A-42" prefix="IC">
<description>&lt;b&gt;HCS08 Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC9S08GT16A.pdf</description>
<gates>
<gate name="G$1" symbol="MC9S08GT16A-42"/>
</gates>
<devices>
<device name="" package="PSDIP_42">
<connects>
<connect gate="G$1" pin="!RESET" pad="6"/>
<connect gate="G$1" pin="IRQ" pad="14"/>
<connect gate="G$1" pin="PTA0/KBIP0" pad="35"/>
<connect gate="G$1" pin="PTA1/KBIP1" pad="36"/>
<connect gate="G$1" pin="PTA2/KBIP2" pad="37"/>
<connect gate="G$1" pin="PTA3/KBIP3" pad="38"/>
<connect gate="G$1" pin="PTA4/KBIP4" pad="39"/>
<connect gate="G$1" pin="PTA5/KBIP5" pad="40"/>
<connect gate="G$1" pin="PTA6/KBIP6" pad="41"/>
<connect gate="G$1" pin="PTA7/KBIP7" pad="42"/>
<connect gate="G$1" pin="PTB0/ADP0" pad="25"/>
<connect gate="G$1" pin="PTB1/ADP1" pad="26"/>
<connect gate="G$1" pin="PTB2/ADP2" pad="27"/>
<connect gate="G$1" pin="PTB3/ADP3" pad="28"/>
<connect gate="G$1" pin="PTB4/ADP4" pad="29"/>
<connect gate="G$1" pin="PTB5/ADP5" pad="30"/>
<connect gate="G$1" pin="PTB6/ADP6" pad="31"/>
<connect gate="G$1" pin="PTB7/ADP7" pad="32"/>
<connect gate="G$1" pin="PTC0/TXD2" pad="7"/>
<connect gate="G$1" pin="PTC1/RXD2" pad="8"/>
<connect gate="G$1" pin="PTC2/SDA" pad="9"/>
<connect gate="G$1" pin="PTC3/SCL" pad="10"/>
<connect gate="G$1" pin="PTC4" pad="11"/>
<connect gate="G$1" pin="PTD0/TPM1CLK/TPM1CH0" pad="21"/>
<connect gate="G$1" pin="PTD1/TPM1CH1" pad="22"/>
<connect gate="G$1" pin="PTD3/TPM2CLK/TPM2CH0" pad="23"/>
<connect gate="G$1" pin="PTD4/TPM2CH1" pad="24"/>
<connect gate="G$1" pin="PTE0/TXD1" pad="12"/>
<connect gate="G$1" pin="PTE1/RXD1" pad="13"/>
<connect gate="G$1" pin="PTE2/!SS" pad="15"/>
<connect gate="G$1" pin="PTE3/MISO" pad="16"/>
<connect gate="G$1" pin="PTE4/MOSI" pad="17"/>
<connect gate="G$1" pin="PTE5/SPSCK" pad="18"/>
<connect gate="G$1" pin="PTG0/BKGD/MS" pad="3"/>
<connect gate="G$1" pin="PTG1/XTAL" pad="4"/>
<connect gate="G$1" pin="PTG2/EXTAL" pad="5"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VDDAD" pad="1"/>
<connect gate="G$1" pin="VREFH" pad="33"/>
<connect gate="G$1" pin="VREFL" pad="34"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="VSSAD" pad="2"/>
</connects>
<technologies>
<technology name="16">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC9S08GT16ACBE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="01M5858"/>
</technology>
<technology name="8">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC9S08GT8ACBE"/>
<attribute name="OC_FARNELL" value="1294366"/>
<attribute name="OC_NEWARK" value="01M5868"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC9S08GT*A-32" prefix="IC">
<description>&lt;b&gt;HCS08 Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/microcontrollers/doc/data_sheet/MC9S08GT16A.pdf</description>
<gates>
<gate name="G$1" symbol="MC9S08GT16A-32"/>
</gates>
<devices>
<device name="" package="QFN32">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="IRQ" pad="8"/>
<connect gate="G$1" pin="PTA4/KBIP4" pad="24"/>
<connect gate="G$1" pin="PTA5/KBIP5" pad="25"/>
<connect gate="G$1" pin="PTA6/KBIP6" pad="26"/>
<connect gate="G$1" pin="PTA7/KBIP7" pad="27"/>
<connect gate="G$1" pin="PTB0/ADP0" pad="18"/>
<connect gate="G$1" pin="PTB1/ADP1" pad="19"/>
<connect gate="G$1" pin="PTB2/ADP2" pad="20"/>
<connect gate="G$1" pin="PTB3/ADP3" pad="21"/>
<connect gate="G$1" pin="PTC0/TXD2" pad="2"/>
<connect gate="G$1" pin="PTC1/RXD2" pad="3"/>
<connect gate="G$1" pin="PTC2/SDA" pad="4"/>
<connect gate="G$1" pin="PTC3/SCL" pad="5"/>
<connect gate="G$1" pin="PTD0/TPM1CLK/TPM1CH0" pad="15"/>
<connect gate="G$1" pin="PTD1/TPM1CH1" pad="16"/>
<connect gate="G$1" pin="PTD3/TPM2CLK/TPM2CH0" pad="17"/>
<connect gate="G$1" pin="PTE0/TXD1" pad="6"/>
<connect gate="G$1" pin="PTE1/RXD1" pad="7"/>
<connect gate="G$1" pin="PTE2/!SS" pad="9"/>
<connect gate="G$1" pin="PTE3/MISO" pad="10"/>
<connect gate="G$1" pin="PTE4/MOSI" pad="11"/>
<connect gate="G$1" pin="PTE5/SPSCK" pad="12"/>
<connect gate="G$1" pin="PTG0/BKGD/MS" pad="30"/>
<connect gate="G$1" pin="PTG1/XTAL" pad="31"/>
<connect gate="G$1" pin="PTG2/EXTAL" pad="32"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDDAD" pad="29"/>
<connect gate="G$1" pin="VREFH" pad="22"/>
<connect gate="G$1" pin="VREFL" pad="23"/>
<connect gate="G$1" pin="VSS@1" pad="13"/>
<connect gate="G$1" pin="VSSAD" pad="28"/>
</connects>
<technologies>
<technology name="16">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC9S08GT16ACFCE"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="01M5860"/>
</technology>
<technology name="8">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MC9S08GT8AMFCE"/>
<attribute name="OC_FARNELL" value="1294367"/>
<attribute name="OC_NEWARK" value="01M5873"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
