<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>Infineon Microcontroller &lt;b&gt;TriCore TM&lt;/b&gt; 32-bit MCU-DSP Architecture&lt;p&gt;
Designed by: Alexander Blümel &amp;lt;Schlager_IE_GmbH@t-online.de&amp;gt;&lt;br&gt;
extended by: librarian@cadsoft.de</description>
<packages>
<package name="P-BGA329">
<description>&lt;b&gt;P-BGA-329&lt;/b&gt; Plastic Ball Grid Array Package&lt;p&gt;
Source: http://www.infineon.com</description>
</package>
<package name="P-LBGA-260">
<description>&lt;b&gt;P-LBGA-260&lt;/b&gt; Plastic Ball Grid Array Package&lt;p&gt;
Source: http://www.infineon.com</description>
</package>
<package name="P-LBGA-208-2">
<description>&lt;b&gt;P-LBGA-208-2&lt;/b&gt; Low Profile Plastic Ball Grid Array Package&lt;p&gt;
Source: http://www.infineon.com .. TC1130_DS_v031.pdf</description>
</package>
<package name="LOGO_5MM">
<description>&lt;b&gt;Infineon Logo&lt;/b&gt;</description>
</package>
<package name="P-BGA-388-2">
<description>&lt;b&gt;P-BGA-388&lt;/b&gt; Plastic Ball Grid Array Package&lt;p&gt;
Source: www.infenon.com .. gpa09218.eps.ps</description>
</package>
<package name="FQFP208-2">
<description>&lt;b&gt;P-FQFP-208-2, -4, -7&lt;/b&gt; Plastic Fine Pitch Quad Flat Package&lt;p&gt;
Source: http://www.infineon.com</description>
</package>
</packages>
<symbols>
<symbol name="TC10">
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="out" function="clk"/>
<pin name="P0.1"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P0.0"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P2.0"/>
<pin name="P2.1"/>
<pin name="P2.2"/>
<pin name="P2.3"/>
<pin name="P2.4"/>
<pin name="P2.5"/>
<pin name="P2.6"/>
<pin name="P2.7"/>
<pin name="/RD" direction="out" function="dot"/>
<pin name="/WR" direction="out" function="dot"/>
<pin name="/BREQ" direction="out" function="dot"/>
<pin name="/HOLD" direction="out" function="dot"/>
<pin name="/HLDA" direction="out" function="dot"/>
<pin name="ALE" direction="out"/>
<pin name="NMI" direction="in" function="dot"/>
<pin name="/HRST" direction="in" function="dot"/>
<pin name="/POR" direction="in" function="dot"/>
<pin name="/CODE" direction="out" function="dot"/>
<pin name="/CAS" direction="out" function="dot"/>
<pin name="/RAS" direction="out" function="dot"/>
<pin name="/CSFPI" direction="out" function="dot"/>
<pin name="/WAIT" direction="out" function="dot"/>
<pin name="/CSOL" direction="out" function="dot"/>
<pin name="/CSFM" direction="out" function="dot"/>
<pin name="EBUC" direction="out"/>
<pin name="STATUS0"/>
<pin name="STATUS1"/>
<pin name="STATUS2"/>
<pin name="STATUS3"/>
<pin name="STATUS4"/>
<pin name="BRKPT0"/>
<pin name="BRKPT1"/>
<pin name="BRKPT2"/>
<pin name="IND_PC0"/>
<pin name="IND_PC1"/>
<pin name="IND_PC2"/>
<pin name="IND_PC3"/>
<pin name="IND_PC4"/>
<pin name="IND_PC5"/>
<pin name="IND_PC6"/>
<pin name="IND_PC7"/>
<pin name="PCP_PC0"/>
<pin name="PCP_PC1"/>
<pin name="PCP_PC2"/>
<pin name="PCP_PC3"/>
<pin name="PCP_PC4"/>
<pin name="PCP_PC5"/>
<pin name="PCP_PC6"/>
<pin name="PCP_PC7"/>
<pin name="PCP_PC8"/>
<pin name="BC0"/>
<pin name="BC1"/>
<pin name="BC2"/>
<pin name="BC3"/>
<pin name="CS0" direction="out" function="dot"/>
<pin name="CS1" direction="out" function="dot"/>
<pin name="CS2" direction="out" function="dot"/>
<pin name="CS3" direction="out" function="dot"/>
<pin name="CLKS@0" direction="in" function="clk"/>
<pin name="CLKS@1" direction="in" function="clk"/>
<pin name="CLKS@2" direction="in" function="clk"/>
<pin name="SCAN@0" direction="in"/>
<pin name="SCAN@1" direction="in"/>
<pin name="VCOS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in" function="dot"/>
<pin name="BYPASS"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="OCDS_E" direction="out" function="dot"/>
<pin name="BRK_OUT" direction="out" function="dot"/>
<pin name="(CHIPZ)"/>
</symbol>
<symbol name="VSS_VDD">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="VSSE_VDD">
<pin name="VDDE" direction="pwr"/>
<pin name="VSSE" direction="pwr"/>
</symbol>
<symbol name="VSSP_VDD">
<pin name="VDDP" direction="pwr"/>
<pin name="VSSP" direction="pwr"/>
</symbol>
<symbol name="TC1775">
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="XTAL3" function="clk"/>
<pin name="XTAL4" function="clk"/>
<pin name="TESTMODE" function="dot"/>
<pin name="CLKIN" direction="in" function="clk"/>
<pin name="CLKOUT" direction="out" function="clk"/>
<pin name="HDRST" function="dot"/>
<pin name="PORST" direction="in" function="dot"/>
<pin name="NMI" direction="in" function="dot"/>
<pin name="CFG0" direction="in"/>
<pin name="CFG1" direction="in"/>
<pin name="CFG2" direction="in"/>
<pin name="CFG3" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="CLKSEL0" direction="in"/>
<pin name="CLKSEL1" direction="in"/>
<pin name="CLKSEL2" direction="in"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VAREF@0" direction="pwr"/>
<pin name="VAREF@1" direction="pwr"/>
<pin name="VAGND@0" direction="pwr"/>
<pin name="VAGND@1" direction="pwr"/>
<pin name="VDDA@0" direction="pwr"/>
<pin name="VDDA@1" direction="pwr"/>
<pin name="VSSA@0" direction="pwr"/>
<pin name="VSSA@1" direction="pwr"/>
</symbol>
<symbol name="PORT16">
<pin name="0" direction="in"/>
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="6" direction="in"/>
<pin name="7" direction="in"/>
<pin name="8" direction="in"/>
<pin name="9" direction="in"/>
<pin name="10" direction="in"/>
<pin name="11" direction="in"/>
<pin name="12" direction="in"/>
<pin name="13" direction="in"/>
<pin name="14" direction="in"/>
<pin name="15" direction="in"/>
</symbol>
<symbol name="NC10">
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
</symbol>
<symbol name="JTAG-OCSD">
<pin name="!TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="!OCDSE" direction="in"/>
<pin name="!BRKIN" direction="in"/>
<pin name="!BRKOUT" direction="out"/>
</symbol>
<symbol name="VSS">
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="D31">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D16"/>
<pin name="D17"/>
<pin name="D18"/>
<pin name="D19"/>
<pin name="D20"/>
<pin name="D21"/>
<pin name="D22"/>
<pin name="D23"/>
<pin name="D24"/>
<pin name="D25"/>
<pin name="D26"/>
<pin name="D27"/>
<pin name="D28"/>
<pin name="D29"/>
<pin name="D30"/>
<pin name="D31"/>
</symbol>
<symbol name="A23">
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
</symbol>
<symbol name="AN23">
<pin name="AN0" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AN3" direction="in"/>
<pin name="AN4" direction="in"/>
<pin name="AN5" direction="in"/>
<pin name="AN6" direction="in"/>
<pin name="AN7" direction="in"/>
<pin name="AN8" direction="in"/>
<pin name="AN9" direction="in"/>
<pin name="AN10" direction="in"/>
<pin name="AN11" direction="in"/>
<pin name="AN12" direction="in"/>
<pin name="AN13" direction="in"/>
<pin name="AN14" direction="in"/>
<pin name="AN15" direction="in"/>
<pin name="AN16" direction="in"/>
<pin name="AN17" direction="in"/>
<pin name="AN18" direction="in"/>
<pin name="AN19" direction="in"/>
<pin name="AN20" direction="in"/>
<pin name="AN21" direction="in"/>
<pin name="AN22" direction="in"/>
<pin name="AN23" direction="in"/>
</symbol>
<symbol name="TC1765">
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="ECIN"/>
<pin name="ECOUT"/>
<pin name="RD" function="dot"/>
<pin name="RD/!WR" function="dot"/>
<pin name="ADV" function="dot"/>
<pin name="/BC0" function="dot"/>
<pin name="/BC1" function="dot"/>
<pin name="/BC2" function="dot"/>
<pin name="/BC3" function="dot"/>
<pin name="/BAA" function="dot"/>
<pin name="/CODE" function="dot"/>
<pin name="/CS0" function="dot"/>
<pin name="/CS1" function="dot"/>
<pin name="/CS2" function="dot"/>
<pin name="/CS3" function="dot"/>
<pin name="/WAIT/!IND" function="dot"/>
<pin name="/CDEMU/!CSOVK" function="dot"/>
<pin name="CPUCLK" function="clk"/>
<pin name="/NMI" function="dot"/>
<pin name="/TEST/MODE" function="dot"/>
<pin name="/HDRST" function="dot"/>
<pin name="BYPASS"/>
<pin name="/PO_RST" function="dot"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.4"/>
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
</symbol>
<symbol name="GND6">
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
</symbol>
<symbol name="TC1130">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16"/>
<pin name="A17"/>
<pin name="A18"/>
<pin name="A19"/>
<pin name="A20"/>
<pin name="A21"/>
<pin name="A22"/>
<pin name="A23"/>
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="NMI"/>
<pin name="/RD" function="dot"/>
<pin name="/WR" function="dot"/>
<pin name="CS0" function="dot"/>
<pin name="CS1" function="dot"/>
<pin name="CS2" function="dot"/>
<pin name="CS3" function="dot"/>
<pin name="BC0" function="dot"/>
<pin name="BC1" function="dot"/>
<pin name="BC2" function="dot"/>
<pin name="BC3" function="dot"/>
<pin name="/PORST" function="dot"/>
<pin name="/HDRST" function="dot"/>
<pin name="HWCFG0"/>
<pin name="HWCFG1"/>
<pin name="HWCFG2"/>
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="VDDOSC"/>
<pin name="VDDOSC3"/>
<pin name="VSSOSC3"/>
<pin name="VSSOSC"/>
<pin name="/WAIT" function="dot"/>
<pin name="/MR_W" function="dot"/>
<pin name="BFCLKI"/>
<pin name="BFCLKO"/>
<pin name="ALE"/>
<pin name="/BAA" function="dot"/>
<pin name="/ADV" function="dot"/>
<pin name="/CSCOMB" function="dot"/>
<pin name="CKE"/>
<pin name="/RAS" function="dot"/>
<pin name="/CAS" function="dot"/>
<pin name="SDCLKI"/>
<pin name="SDCLKO"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="TRST"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="/BRKIN" function="dot"/>
<pin name="TRCLK"/>
<pin name="MI_TXCLK"/>
<pin name="MI_RXCLK"/>
<pin name="MI_MDIO"/>
</symbol>
<symbol name="PWR_TC1130">
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDDP@0" direction="pwr"/>
<pin name="VDDP@1" direction="pwr"/>
<pin name="VDDP@2" direction="pwr"/>
<pin name="VDDP@3" direction="pwr"/>
<pin name="VDDP@4" direction="pwr"/>
<pin name="VDDP@5" direction="pwr"/>
</symbol>
<symbol name="NC4">
<pin name="RESERVED@0" direction="nc"/>
<pin name="RESERVED@1" direction="nc"/>
<pin name="RESERVED@2" direction="nc"/>
<pin name="RESERVED@3" direction="nc"/>
</symbol>
<symbol name="TC1912">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16"/>
<pin name="A17"/>
<pin name="A18"/>
<pin name="A19"/>
<pin name="A20"/>
<pin name="A21"/>
<pin name="A22"/>
<pin name="A23"/>
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="NMI"/>
<pin name="/RD" function="dot"/>
<pin name="/WR" function="dot"/>
<pin name="CS0" function="dot"/>
<pin name="CS1" function="dot"/>
<pin name="CS2" function="dot"/>
<pin name="CS3" function="dot"/>
<pin name="BC0" function="dot"/>
<pin name="BC1" function="dot"/>
<pin name="BC2" function="dot"/>
<pin name="BC3" function="dot"/>
<pin name="/PORST" function="dot"/>
<pin name="/HDRST" function="dot"/>
<pin name="HWCFG0"/>
<pin name="HWCFG1"/>
<pin name="HWCFG2"/>
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="VDDOSC"/>
<pin name="VDDOSC3"/>
<pin name="VSSOSC3"/>
<pin name="VSSOSC"/>
<pin name="/WAIT" function="dot"/>
<pin name="/MR_W" function="dot"/>
<pin name="BFCLKI"/>
<pin name="BFCLKO"/>
<pin name="ALE"/>
<pin name="/BAA" function="dot"/>
<pin name="/ADV" function="dot"/>
<pin name="/CSCOMB" function="dot"/>
<pin name="CKE"/>
<pin name="/RAS" function="dot"/>
<pin name="/CAS" function="dot"/>
<pin name="SDCLKI"/>
<pin name="SDCLKO"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="TRST"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="/BRKIN" function="dot"/>
<pin name="TRCLK"/>
<pin name="MI_TXCLK"/>
<pin name="MI_RXCLK"/>
<pin name="MI_MDIO"/>
</symbol>
<symbol name="TC1920">
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="XTAL3" function="clk"/>
<pin name="XTAL4" function="clk"/>
<pin name="CLKOUT" direction="out" function="clk"/>
<pin name="HRST" function="dot"/>
<pin name="PORST" direction="in" function="dot"/>
<pin name="NMI" direction="in" function="dot"/>
<pin name="BYPASS" direction="in"/>
<pin name="VDD_OSC2" direction="pwr"/>
<pin name="VDD_OSC1" direction="pwr"/>
<pin name="VDDP_OSC" direction="pwr"/>
<pin name="VSS_OSC" direction="pwr"/>
<pin name="CS0" function="dot"/>
<pin name="CS1" function="dot"/>
<pin name="CS2" function="dot"/>
<pin name="CS3" function="dot"/>
<pin name="CS4" function="dot"/>
<pin name="CS5" function="dot"/>
<pin name="CS6" function="dot"/>
<pin name="CSEMU" function="dot"/>
<pin name="CSOVL" function="dot"/>
<pin name="/BC0" function="dot"/>
<pin name="/BC1" function="dot"/>
<pin name="/BC2" function="dot"/>
<pin name="/BC3" function="dot"/>
<pin name="/RD" function="dot"/>
<pin name="/WR" function="dot"/>
<pin name="ALE"/>
<pin name="/WAIT" function="dot"/>
<pin name="/BAA" function="dot"/>
<pin name="EBUCLK"/>
<pin name="BFCLK0"/>
<pin name="/CSGLB" function="dot"/>
<pin name="/CMDELAY" function="dot"/>
<pin name="MR/W" function="dot"/>
<pin name="CKE"/>
<pin name="/RAS" function="dot"/>
<pin name="/CAS" function="dot"/>
<pin name="P4.0/AIN0"/>
<pin name="P4.1/AIN1"/>
<pin name="P4.2/AIN2"/>
<pin name="P4.3/AIN3"/>
<pin name="P4.4/AIN4"/>
<pin name="P4.5/AIN5"/>
<pin name="/SCAN_MODE" function="dot"/>
<pin name="PLLCTRL_A0"/>
<pin name="TM_CTRL0"/>
<pin name="TM_CTRL1"/>
<pin name="AI0+"/>
<pin name="AI0-"/>
<pin name="AO0+"/>
<pin name="AO0-"/>
<pin name="AI1+"/>
<pin name="AI1-"/>
<pin name="AO1+"/>
<pin name="AO1-"/>
<pin name="CEXT"/>
<pin name="CODEC_DIS"/>
<pin name="/ADV" direction="pwr" function="dot"/>
</symbol>
<symbol name="PORT8">
<pin name="0" direction="in"/>
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="6" direction="in"/>
<pin name="7" direction="in"/>
</symbol>
<symbol name="TC1920PWR">
<pin name="1V8@0" direction="pwr"/>
<pin name="1V8@1" direction="pwr"/>
<pin name="1V8@2" direction="pwr"/>
<pin name="1V8@3" direction="pwr"/>
<pin name="1V8@4" direction="pwr"/>
<pin name="1V8@5" direction="pwr"/>
<pin name="1V8@6" direction="pwr"/>
<pin name="1V8@7" direction="pwr"/>
<pin name="3V3@0" direction="pwr"/>
<pin name="3V3@1" direction="pwr"/>
<pin name="3V3@2" direction="pwr"/>
<pin name="3V3@3" direction="pwr"/>
<pin name="3V3@4" direction="pwr"/>
<pin name="3V3@5" direction="pwr"/>
<pin name="3V3@6" direction="pwr"/>
<pin name="3V3@7" direction="pwr"/>
<pin name="3V3@8" direction="pwr"/>
<pin name="3V3@9" direction="pwr"/>
<pin name="3V3@10" direction="pwr"/>
<pin name="3V3@11" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
</symbol>
<symbol name="TC1920PWR2">
<pin name="VDDR@0" direction="pwr"/>
<pin name="VDDR@1" direction="pwr"/>
<pin name="VDD_SB" direction="pwr"/>
<pin name="VDD_GUARD" direction="pwr"/>
<pin name="VSS_GUARD@1" direction="pwr"/>
<pin name="VSS_GUARD@2" direction="pwr"/>
<pin name="VGND_COD" direction="pwr"/>
<pin name="VREF_COD" direction="pwr"/>
<pin name="VSSP_COD@0" direction="pwr"/>
<pin name="VSSP_OSC@0" direction="pwr"/>
<pin name="VSSA_COD@0" direction="pwr"/>
<pin name="VSSP_OSC@1" direction="pwr"/>
<pin name="VDDP_COD@0" direction="pwr"/>
<pin name="VDDP_OSC@1" direction="pwr"/>
<pin name="VAGND_ADC" direction="pwr"/>
<pin name="VAREF_ADC" direction="pwr"/>
<pin name="VSSA_ADC" direction="pwr"/>
<pin name="VSSP_ADC@0" direction="pwr"/>
<pin name="VSSP_ADC@1" direction="pwr"/>
<pin name="VSSP_ADC@2" direction="pwr"/>
<pin name="VDDP_ADC" direction="pwr"/>
<pin name="VSS_PLL" direction="pwr"/>
<pin name="VDD_PLL" direction="pwr"/>
</symbol>
<symbol name="TC11IB">
<pin name="CPUCLK" direction="out"/>
<pin name="!NMI" direction="in"/>
<pin name="!RD"/>
<pin name="RESERVED@2"/>
<pin name="!CS0" direction="out"/>
<pin name="!PORST" direction="in"/>
<pin name="!HDRST"/>
<pin name="CFG0"/>
<pin name="!WAIT"/>
<pin name="!MR_W" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!BAA" direction="out"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!CS1" direction="out"/>
<pin name="!CS2" direction="out"/>
<pin name="!CS3" direction="out"/>
<pin name="!CS4" direction="out"/>
<pin name="!CS5" direction="out"/>
<pin name="!CS6" direction="out"/>
<pin name="RESERVED@1" direction="out"/>
<pin name="CFG1"/>
<pin name="CFG2"/>
<pin name="CFG3"/>
<pin name="!SVM" direction="out"/>
<pin name="!HLDA"/>
<pin name="!BREQ" direction="out"/>
<pin name="!CSEMU" direction="out"/>
<pin name="!CSGLB" direction="out"/>
<pin name="!CSOVL" direction="out"/>
<pin name="!CSFPI" direction="out"/>
<pin name="!CKE" direction="out"/>
<pin name="!RMW" direction="out"/>
<pin name="!HOLD" direction="in"/>
<pin name="EBUCLK" direction="out"/>
<pin name="!ADV" direction="out"/>
<pin name="ACLK" direction="out"/>
<pin name="!CMDELAY" direction="in"/>
<pin name="MII_TXCLK" direction="in"/>
<pin name="MII_RXCLK" direction="in"/>
<pin name="MII_MDIO" direction="in"/>
<pin name="TESTMODE" direction="in"/>
<pin name="!TM_CTRL1" direction="in"/>
<pin name="!TM_CTRL2" direction="in"/>
<pin name="CLK42" direction="in"/>
<pin name="PLL96_CTRL" direction="out"/>
<pin name="PLL42_CTRL" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VDDOSC" direction="in"/>
<pin name="VSSOSC" direction="in"/>
<pin name="VDDPLL96" direction="in"/>
<pin name="VSSPLL96" direction="in"/>
<pin name="VDDPLL42" direction="in"/>
<pin name="VSSPLL42" direction="in"/>
<pin name="VLMUREF" direction="in"/>
<pin name="VCOMREF" direction="in"/>
<pin name="!OCDSE" direction="in"/>
<pin name="!BRKIN" direction="in"/>
<pin name="!BRKOUT" direction="out"/>
<pin name="RESERVED@3"/>
<pin name="VDDDRAM@1" direction="in"/>
<pin name="VDDDRAM@2" direction="in"/>
<pin name="RESERVED@4"/>
<pin name="RESERVED@5"/>
<pin name="!BC0"/>
<pin name="!BC1"/>
<pin name="!BC2"/>
<pin name="!BC3"/>
<pin name="!RDWR"/>
</symbol>
<symbol name="AD31">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
</symbol>
<symbol name="PCI">
<pin name="P_PAR"/>
<pin name="!P_SERR"/>
<pin name="!P_PERR"/>
<pin name="!P_STOP"/>
<pin name="!P_DEVSEL"/>
<pin name="!P_TRDY"/>
<pin name="!P_FRAME"/>
<pin name="!P_IRDY"/>
<pin name="!P_LOCK"/>
<pin name="!P_INTA" direction="out"/>
<pin name="!P_INTB" direction="out"/>
<pin name="!P_PME" direction="out"/>
<pin name="!P_REQ" direction="out"/>
<pin name="!P_GNT" direction="in"/>
<pin name="P_IDSEL" direction="in"/>
<pin name="P_CLK33" direction="in"/>
<pin name="!P_CBE0"/>
<pin name="!P_CBE1"/>
<pin name="!P_CBE2"/>
<pin name="!P_CBE3"/>
</symbol>
<symbol name="ODCS/JTAG">
<pin name="!TRST" direction="in"/>
<pin name="OCDS2PS0" direction="out"/>
<pin name="OCDS2PS1" direction="out"/>
<pin name="OCDS2PS2" direction="out"/>
<pin name="OCDS2PS3" direction="out"/>
<pin name="OCDS2PS4" direction="out"/>
<pin name="OCDS2PC0" direction="out"/>
<pin name="OCDS2PC1" direction="out"/>
<pin name="OCDS2PC2" direction="out"/>
<pin name="OCDS2BRK0" direction="out"/>
<pin name="OCDS2BRK1" direction="out"/>
<pin name="OCDS2BRK2" direction="out"/>
<pin name="OCDS2PC3" direction="out"/>
<pin name="OCDS2PC4" direction="out"/>
<pin name="OCDS2PC5" direction="out"/>
<pin name="OCDS2PC6" direction="out"/>
<pin name="OCDS2PC7" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="VDDP">
<pin name="VDDP" direction="pwr"/>
</symbol>
<symbol name="VDD">
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="TC1910">
<pin name="!RD"/>
<pin name="!CS0" direction="out"/>
<pin name="!PORST" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="!WAIT"/>
<pin name="!MR_W" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!BAA" direction="out"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!CS1" direction="out"/>
<pin name="!CS2" direction="out"/>
<pin name="!CS3" direction="out"/>
<pin name="!CS4" direction="out"/>
<pin name="!CS5" direction="out"/>
<pin name="!CS6" direction="out"/>
<pin name="!CSGLB" direction="out"/>
<pin name="CKE" direction="out"/>
<pin name="EBUCLK" direction="out"/>
<pin name="!ADV" direction="out"/>
<pin name="!CMDELAY" direction="in"/>
<pin name="!SCANMODE" direction="in"/>
<pin name="TM_CTRL0" direction="in"/>
<pin name="TM_CTRL1" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="!BC0"/>
<pin name="!BC1"/>
<pin name="!BC2"/>
<pin name="!BC3"/>
<pin name="!RD_WR"/>
<pin name="BFCLK0" direction="out"/>
<pin name="AI0+" direction="in"/>
<pin name="AI0-" direction="in"/>
<pin name="AO0+" direction="out"/>
<pin name="AO0-" direction="out"/>
<pin name="AI1+" direction="in"/>
<pin name="AI1-" direction="in"/>
<pin name="AO1+" direction="out"/>
<pin name="AO1-" direction="out"/>
<pin name="CEXT" direction="in"/>
<pin name="CODEC_DIS" direction="in"/>
<pin name="!CSEMU" direction="out"/>
<pin name="!CSOVL" direction="out"/>
<pin name="PLLCTRL_AO" direction="in"/>
<pin name="XTAL3" direction="in"/>
<pin name="XTAL4" direction="out"/>
<pin name="VAREF_GOD" direction="in"/>
<pin name="VAGND_GOD" direction="in"/>
<pin name="VDD_COD0/1" direction="in"/>
<pin name="VSSA_COD0/1" direction="in"/>
<pin name="VDD_GUARD" direction="in"/>
<pin name="VSS_GUARD" direction="in"/>
<pin name="VDD_OSCI" direction="in"/>
<pin name="VDD_RTC" direction="in"/>
<pin name="VSS_32K" direction="in"/>
<pin name="VDD_PLL" direction="in"/>
<pin name="VSS_PLL" direction="in"/>
<pin name="VDDPLL" direction="in"/>
<pin name="VSSPLL" direction="in"/>
<pin name="VDDR" direction="in"/>
<pin name="VDDSB" direction="in"/>
<pin name="VDD_PWR@1" direction="in"/>
<pin name="VDD_PWR@2" direction="in"/>
<pin name="VDD_PWR@3" direction="in"/>
<pin name="VDD_PWR@4" direction="in"/>
<pin name="VDD_PWR@5" direction="in"/>
<pin name="VDD_PWR2@1" direction="in"/>
<pin name="VDD_PWR2@2" direction="in"/>
<pin name="VDD_PWR2@3" direction="in"/>
<pin name="VDD_PWR2@4" direction="in"/>
<pin name="VSS_GND@1" direction="in"/>
<pin name="VSS_GND@2" direction="in"/>
<pin name="VSS_GND@3" direction="in"/>
<pin name="VSS_GND@4" direction="in"/>
<pin name="VSS_GND@5" direction="in"/>
<pin name="VSS_GND@6" direction="in"/>
<pin name="!NMI" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="!HRST"/>
</symbol>
<symbol name="HEATSINK">
<pin name="HS" direction="in"/>
</symbol>
<symbol name="PORT0-10_12">
<pin name="0/EXI0IN"/>
<pin name="1/EXI1IN/DATA_IN"/>
<pin name="2/EXI2IN/DATA_OUT"/>
<pin name="3/EXI3IN/MCLK"/>
<pin name="4/GPIO/SCLK"/>
<pin name="5/GPIO/LRCK"/>
<pin name="6/GPIO/MUTE0"/>
<pin name="7/GPIO/MUTE1"/>
</symbol>
<symbol name="PORT2-10_12">
<pin name="0/GPIO/RXDCAN0"/>
<pin name="1/GPIO/TXDCAN0"/>
<pin name="2/GPIO/RXDCAN1"/>
<pin name="3/GPIO/TXDCAN1"/>
<pin name="4/GPIO"/>
<pin name="5/GPIO"/>
<pin name="6/SCL"/>
<pin name="7/SDA"/>
<pin name="8/GPIO"/>
<pin name="9/GPIO"/>
<pin name="10/RXD0"/>
<pin name="11/TXD0"/>
<pin name="12/SCLK"/>
<pin name="13/MRST"/>
<pin name="14/MTSR"/>
<pin name="15/GPIO/EXI4IN/PLL_CLC.LOCK"/>
</symbol>
<symbol name="PORT1-10_12">
<pin name="0/GPIO"/>
<pin name="1/GPIO"/>
<pin name="2/GPIO"/>
<pin name="3/GPIO"/>
<pin name="4/GPIO"/>
<pin name="5/GPIO"/>
<pin name="6/GPIO"/>
<pin name="7/GPIO"/>
</symbol>
<symbol name="PORT3-10_12">
<pin name="0/GPTU.0"/>
<pin name="1/GPTU.1"/>
<pin name="2/GPTU.2"/>
<pin name="3/GPTU.3"/>
<pin name="4/GPTU.4"/>
<pin name="5/GPTU.5"/>
<pin name="6/GPTU.6"/>
<pin name="7/GPTU.7"/>
<pin name="8/RXD1"/>
<pin name="9/TXD1"/>
<pin name="10/GPIO/RXD2"/>
<pin name="11/GPIO/OSCBYP/TXD2"/>
<pin name="12/EXI5IN/HWCFG0"/>
<pin name="13/EXI6IN/HWCFG1"/>
<pin name="14/EXI7IN/HWCFG2"/>
<pin name="15/GPIO"/>
</symbol>
<symbol name="TC1100">
<pin name="!NMI" direction="in"/>
<pin name="!RD" direction="out"/>
<pin name="!CS0" direction="out"/>
<pin name="!PORST" direction="in"/>
<pin name="!HDRST"/>
<pin name="HWCFG0" direction="in"/>
<pin name="!WAIT" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="!BAA" direction="out"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!CS1" direction="out"/>
<pin name="!CS2" direction="out"/>
<pin name="!CS3" direction="out"/>
<pin name="!CSCOMB" direction="out"/>
<pin name="CKE" direction="out"/>
<pin name="SDCLKI" direction="in"/>
<pin name="!ADV" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VDDOSC" direction="in"/>
<pin name="VSSOSC" direction="in"/>
<pin name="RESERVED@1" direction="pas"/>
<pin name="!BC0"/>
<pin name="!BC1"/>
<pin name="!BC2"/>
<pin name="!BC3"/>
<pin name="!RD_WR" direction="out"/>
<pin name="HWCFG1" direction="in"/>
<pin name="HWCFG2" direction="in"/>
<pin name="!TRCLK" direction="out"/>
<pin name="SDCLKO" direction="out"/>
<pin name="BFCLKI" direction="in"/>
<pin name="BFCLKO" direction="out"/>
<pin name="VDDOSC3" direction="in"/>
<pin name="VSSOSC3" direction="in"/>
<pin name="!MR_W" direction="out"/>
<pin name="RESERVED@2" direction="pas"/>
<pin name="RESERVED@3" direction="pas"/>
<pin name="RESERVED@4" direction="pas"/>
<pin name="NC@1" direction="pas"/>
<pin name="NC@2" direction="pas"/>
<pin name="NC@3" direction="pas"/>
<pin name="!BRKIN" direction="in"/>
</symbol>
<symbol name="JTAG">
<pin name="!TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TC10" prefix="IC">
<description>&lt;b&gt;+ Obsolete +&lt;/b&gt; TC10 GP TriCore 32bit  Microcontroller+ DSP&lt;p&gt;
Source: http://www.infineon.com ..</description>
<gates>
<gate name="G" symbol="TC10"/>
<gate name="G$2" symbol="VSSE_VDD"/>
<gate name="G$3" symbol="VSSE_VDD"/>
<gate name="G$4" symbol="VSSE_VDD"/>
<gate name="G$5" symbol="VSSE_VDD"/>
<gate name="G$6" symbol="VSSE_VDD"/>
<gate name="G$7" symbol="VSSE_VDD"/>
<gate name="G$8" symbol="VSSE_VDD"/>
<gate name="G$9" symbol="VSSE_VDD"/>
<gate name="G$10" symbol="VSSE_VDD"/>
<gate name="G$11" symbol="VSSE_VDD"/>
<gate name="G$12" symbol="VSSE_VDD"/>
<gate name="G$13" symbol="VSSE_VDD"/>
<gate name="G$14" symbol="VSSE_VDD"/>
<gate name="G$15" symbol="VSSE_VDD"/>
<gate name="G$16" symbol="VSSE_VDD"/>
<gate name="G$17" symbol="VSSE_VDD"/>
<gate name="G$18" symbol="VSSE_VDD"/>
<gate name="G$19" symbol="VSSE_VDD"/>
<gate name="G$20" symbol="VSSE_VDD"/>
<gate name="G$21" symbol="VSS_VDD"/>
<gate name="G$22" symbol="VSS_VDD"/>
<gate name="G$23" symbol="VSS_VDD"/>
<gate name="G$24" symbol="VSS_VDD"/>
<gate name="G$25" symbol="VSS_VDD"/>
<gate name="G$26" symbol="VSS_VDD"/>
<gate name="G$27" symbol="VSS_VDD"/>
<gate name="G$28" symbol="VSSP_VDD"/>
<gate name="G$1" symbol="VSSE_VDD"/>
<gate name="G$29" symbol="VSS_VDD"/>
</gates>
<devices>
<device name="" package="FQFP208-2">
<connects>
<connect gate="G" pin="(CHIPZ)" pad="54"/>
<connect gate="G" pin="/BREQ" pad="105"/>
<connect gate="G" pin="/CAS" pad="153"/>
<connect gate="G" pin="/CODE" pad="152"/>
<connect gate="G" pin="/CSFM" pad="161"/>
<connect gate="G" pin="/CSFPI" pad="157"/>
<connect gate="G" pin="/CSOL" pad="160"/>
<connect gate="G" pin="/HLDA" pad="104"/>
<connect gate="G" pin="/HOLD" pad="103"/>
<connect gate="G" pin="/HRST" pad="51"/>
<connect gate="G" pin="/POR" pad="52"/>
<connect gate="G" pin="/RAS" pad="154"/>
<connect gate="G" pin="/RD" pad="156"/>
<connect gate="G" pin="/WAIT" pad="158"/>
<connect gate="G" pin="/WR" pad="155"/>
<connect gate="G" pin="A0" pad="177"/>
<connect gate="G" pin="A1" pad="178"/>
<connect gate="G" pin="A10" pad="189"/>
<connect gate="G" pin="A11" pad="190"/>
<connect gate="G" pin="A12" pad="191"/>
<connect gate="G" pin="A13" pad="196"/>
<connect gate="G" pin="A14" pad="197"/>
<connect gate="G" pin="A15" pad="198"/>
<connect gate="G" pin="A16" pad="199"/>
<connect gate="G" pin="A17" pad="200"/>
<connect gate="G" pin="A18" pad="201"/>
<connect gate="G" pin="A19" pad="204"/>
<connect gate="G" pin="A2" pad="179"/>
<connect gate="G" pin="A20" pad="205"/>
<connect gate="G" pin="A21" pad="206"/>
<connect gate="G" pin="A22" pad="207"/>
<connect gate="G" pin="A23" pad="208"/>
<connect gate="G" pin="A3" pad="180"/>
<connect gate="G" pin="A4" pad="181"/>
<connect gate="G" pin="A5" pad="184"/>
<connect gate="G" pin="A6" pad="185"/>
<connect gate="G" pin="A7" pad="186"/>
<connect gate="G" pin="A8" pad="187"/>
<connect gate="G" pin="A9" pad="188"/>
<connect gate="G" pin="AD0" pad="149"/>
<connect gate="G" pin="AD1" pad="148"/>
<connect gate="G" pin="AD10" pad="135"/>
<connect gate="G" pin="AD11" pad="134"/>
<connect gate="G" pin="AD12" pad="133"/>
<connect gate="G" pin="AD13" pad="132"/>
<connect gate="G" pin="AD14" pad="129"/>
<connect gate="G" pin="AD15" pad="128"/>
<connect gate="G" pin="AD16" pad="127"/>
<connect gate="G" pin="AD17" pad="126"/>
<connect gate="G" pin="AD18" pad="125"/>
<connect gate="G" pin="AD19" pad="124"/>
<connect gate="G" pin="AD2" pad="147"/>
<connect gate="G" pin="AD20" pad="123"/>
<connect gate="G" pin="AD21" pad="122"/>
<connect gate="G" pin="AD22" pad="117"/>
<connect gate="G" pin="AD23" pad="116"/>
<connect gate="G" pin="AD24" pad="115"/>
<connect gate="G" pin="AD25" pad="114"/>
<connect gate="G" pin="AD26" pad="113"/>
<connect gate="G" pin="AD27" pad="112"/>
<connect gate="G" pin="AD28" pad="109"/>
<connect gate="G" pin="AD29" pad="108"/>
<connect gate="G" pin="AD3" pad="146"/>
<connect gate="G" pin="AD30" pad="107"/>
<connect gate="G" pin="AD31" pad="106"/>
<connect gate="G" pin="AD4" pad="145"/>
<connect gate="G" pin="AD5" pad="144"/>
<connect gate="G" pin="AD6" pad="139"/>
<connect gate="G" pin="AD7" pad="138"/>
<connect gate="G" pin="AD8" pad="137"/>
<connect gate="G" pin="AD9" pad="136"/>
<connect gate="G" pin="ALE" pad="159"/>
<connect gate="G" pin="BC0" pad="169"/>
<connect gate="G" pin="BC1" pad="174"/>
<connect gate="G" pin="BC2" pad="175"/>
<connect gate="G" pin="BC3" pad="176"/>
<connect gate="G" pin="BRKPT0" pad="60"/>
<connect gate="G" pin="BRKPT1" pad="57"/>
<connect gate="G" pin="BRKPT2" pad="56"/>
<connect gate="G" pin="BRK_OUT" pad="55"/>
<connect gate="G" pin="BYPASS" pad="84"/>
<connect gate="G" pin="CLKS@0" pad="11"/>
<connect gate="G" pin="CLKS@1" pad="12"/>
<connect gate="G" pin="CLKS@2" pad="13"/>
<connect gate="G" pin="CS0" pad="165"/>
<connect gate="G" pin="CS1" pad="166"/>
<connect gate="G" pin="CS2" pad="167"/>
<connect gate="G" pin="CS3" pad="168"/>
<connect gate="G" pin="EBUC" pad="163"/>
<connect gate="G" pin="IND_PC0" pad="74"/>
<connect gate="G" pin="IND_PC1" pad="75"/>
<connect gate="G" pin="IND_PC2" pad="76"/>
<connect gate="G" pin="IND_PC3" pad="77"/>
<connect gate="G" pin="IND_PC4" pad="80"/>
<connect gate="G" pin="IND_PC5" pad="81"/>
<connect gate="G" pin="IND_PC6" pad="82"/>
<connect gate="G" pin="IND_PC7" pad="83"/>
<connect gate="G" pin="NC@0" pad="85"/>
<connect gate="G" pin="NC@1" pad="86"/>
<connect gate="G" pin="NC@2" pad="87"/>
<connect gate="G" pin="NMI" pad="50"/>
<connect gate="G" pin="OCDS_E" pad="53"/>
<connect gate="G" pin="P0.0" pad="18"/>
<connect gate="G" pin="P0.1" pad="19"/>
<connect gate="G" pin="P0.2" pad="20"/>
<connect gate="G" pin="P0.3" pad="21"/>
<connect gate="G" pin="P0.4" pad="22"/>
<connect gate="G" pin="P0.5" pad="23"/>
<connect gate="G" pin="P0.6" pad="24"/>
<connect gate="G" pin="P0.7" pad="25"/>
<connect gate="G" pin="P1.0" pad="28"/>
<connect gate="G" pin="P1.1" pad="29"/>
<connect gate="G" pin="P1.2" pad="30"/>
<connect gate="G" pin="P1.3" pad="31"/>
<connect gate="G" pin="P1.4" pad="32"/>
<connect gate="G" pin="P1.5" pad="33"/>
<connect gate="G" pin="P1.6" pad="34"/>
<connect gate="G" pin="P1.7" pad="35"/>
<connect gate="G" pin="P2.0" pad="40"/>
<connect gate="G" pin="P2.1" pad="41"/>
<connect gate="G" pin="P2.2" pad="42"/>
<connect gate="G" pin="P2.3" pad="43"/>
<connect gate="G" pin="P2.4" pad="44"/>
<connect gate="G" pin="P2.5" pad="45"/>
<connect gate="G" pin="P2.6" pad="48"/>
<connect gate="G" pin="P2.7" pad="49"/>
<connect gate="G" pin="PCP_PC0" pad="102"/>
<connect gate="G" pin="PCP_PC1" pad="101"/>
<connect gate="G" pin="PCP_PC2" pad="100"/>
<connect gate="G" pin="PCP_PC3" pad="97"/>
<connect gate="G" pin="PCP_PC4" pad="96"/>
<connect gate="G" pin="PCP_PC5" pad="95"/>
<connect gate="G" pin="PCP_PC6" pad="94"/>
<connect gate="G" pin="PCP_PC7" pad="93"/>
<connect gate="G" pin="PCP_PC8" pad="92"/>
<connect gate="G" pin="SCAN@0" pad="8"/>
<connect gate="G" pin="SCAN@1" pad="9"/>
<connect gate="G" pin="STATUS0" pad="65"/>
<connect gate="G" pin="STATUS1" pad="64"/>
<connect gate="G" pin="STATUS2" pad="63"/>
<connect gate="G" pin="STATUS3" pad="62"/>
<connect gate="G" pin="STATUS4" pad="61"/>
<connect gate="G" pin="TCK" pad="2"/>
<connect gate="G" pin="TDI" pad="4"/>
<connect gate="G" pin="TDO" pad="5"/>
<connect gate="G" pin="TMS" pad="3"/>
<connect gate="G" pin="TRST" pad="1"/>
<connect gate="G" pin="VCOS" pad="10"/>
<connect gate="G" pin="XTAL1" pad="71"/>
<connect gate="G" pin="XTAL2" pad="70"/>
<connect gate="G$1" pin="VDDE" pad="6"/>
<connect gate="G$1" pin="VSSE" pad="7"/>
<connect gate="G$10" pin="VDDE" pad="118"/>
<connect gate="G$10" pin="VSSE" pad="119"/>
<connect gate="G$11" pin="VDDE" pad="130"/>
<connect gate="G$11" pin="VSSE" pad="131"/>
<connect gate="G$12" pin="VDDE" pad="140"/>
<connect gate="G$12" pin="VSSE" pad="141"/>
<connect gate="G$13" pin="VDDE" pad="150"/>
<connect gate="G$13" pin="VSSE" pad="151"/>
<connect gate="G$14" pin="VDDE" pad="162"/>
<connect gate="G$14" pin="VSSE" pad="164"/>
<connect gate="G$15" pin="VDDE" pad="170"/>
<connect gate="G$15" pin="VSSE" pad="171"/>
<connect gate="G$16" pin="VDDE" pad="182"/>
<connect gate="G$16" pin="VSSE" pad="183"/>
<connect gate="G$17" pin="VDDE" pad="202"/>
<connect gate="G$17" pin="VSSE" pad="203"/>
<connect gate="G$18" pin="VDDE" pad="46"/>
<connect gate="G$18" pin="VSSE" pad="47"/>
<connect gate="G$19" pin="VDDE" pad="58"/>
<connect gate="G$19" pin="VSSE" pad="59"/>
<connect gate="G$2" pin="VDDE" pad="14"/>
<connect gate="G$2" pin="VSSE" pad="15"/>
<connect gate="G$20" pin="VDDE" pad="192"/>
<connect gate="G$20" pin="VSSE" pad="193"/>
<connect gate="G$21" pin="VDD" pad="17"/>
<connect gate="G$21" pin="VSS" pad="16"/>
<connect gate="G$22" pin="VDD" pad="39"/>
<connect gate="G$22" pin="VSS" pad="38"/>
<connect gate="G$23" pin="VDD" pad="69"/>
<connect gate="G$23" pin="VSS" pad="68"/>
<connect gate="G$24" pin="VDD" pad="91"/>
<connect gate="G$24" pin="VSS" pad="90"/>
<connect gate="G$25" pin="VDD" pad="121"/>
<connect gate="G$25" pin="VSS" pad="120"/>
<connect gate="G$26" pin="VDD" pad="143"/>
<connect gate="G$26" pin="VSS" pad="142"/>
<connect gate="G$27" pin="VDD" pad="173"/>
<connect gate="G$27" pin="VSS" pad="172"/>
<connect gate="G$28" pin="VDDP" pad="73"/>
<connect gate="G$28" pin="VSSP" pad="72"/>
<connect gate="G$29" pin="VDD" pad="195"/>
<connect gate="G$29" pin="VSS" pad="194"/>
<connect gate="G$3" pin="VDDE" pad="26"/>
<connect gate="G$3" pin="VSSE" pad="27"/>
<connect gate="G$4" pin="VDDE" pad="36"/>
<connect gate="G$4" pin="VSSE" pad="37"/>
<connect gate="G$5" pin="VDDE" pad="66"/>
<connect gate="G$5" pin="VSSE" pad="67"/>
<connect gate="G$6" pin="VDDE" pad="78"/>
<connect gate="G$6" pin="VSSE" pad="79"/>
<connect gate="G$7" pin="VDDE" pad="88"/>
<connect gate="G$7" pin="VSSE" pad="89"/>
<connect gate="G$8" pin="VDDE" pad="98"/>
<connect gate="G$8" pin="VSSE" pad="99"/>
<connect gate="G$9" pin="VDDE" pad="110"/>
<connect gate="G$9" pin="VSSE" pad="111"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1775" prefix="IC">
<description>&lt;b&gt;TC1775 (AUDO1)&lt;/b&gt; 32-bit microcontroller&lt;p&gt;
for high demanding automotive and industrial applications&lt;br&gt;
(e.g. engine management, starter generator, 3-phase motor control or robotics) &lt;br&gt;
Source: http://www.infineon.com ..</description>
<gates>
<gate name="PORT12" symbol="PORT16"/>
<gate name="PORT13" symbol="PORT16"/>
<gate name="P8/GPTA" symbol="PORT16"/>
<gate name="P9/GPTA" symbol="PORT16"/>
<gate name="PORT10" symbol="PORT16"/>
<gate name="PORT11" symbol="PORT16"/>
<gate name="P5/TRACE" symbol="PORT16"/>
<gate name="P6/ADC0" symbol="PORT16"/>
<gate name="P7/ADC1" symbol="PORT16"/>
<gate name="AD0-15" symbol="PORT16"/>
<gate name="AD16-31" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="P3" symbol="PORT16"/>
<gate name="P4" symbol="PORT16"/>
<gate name="NC" symbol="NC10"/>
<gate name="PWR1-2.5V" symbol="VSS_VDD"/>
<gate name="PWR2-2.5V" symbol="VSS_VDD"/>
<gate name="PWR3-2.5V" symbol="VSS_VDD"/>
<gate name="PWR4-2.5V" symbol="VSS_VDD"/>
<gate name="PWR5-2.5V" symbol="VSS_VDD"/>
<gate name="PWR6-3.3V" symbol="VSS_VDD"/>
<gate name="PWR7-3.3V" symbol="VSS_VDD"/>
<gate name="PWR8-3.3V" symbol="VSS_VDD"/>
<gate name="PWR9-3.3V" symbol="VSS_VDD"/>
<gate name="PWR10-3.3V" symbol="VSS_VDD"/>
<gate name="PWR11-3.3V" symbol="VSS_VDD"/>
<gate name="PWR12-2.5V" symbol="VSS_VDD"/>
<gate name="PWR13-2.5V" symbol="VSS_VDD"/>
<gate name="PWR14-2.5V" symbol="VSS_VDD"/>
<gate name="PWR15-2.5V" symbol="VSS_VDD"/>
<gate name="P-SB-2.5V" symbol="VSS_VDD"/>
<gate name="P-SRAM1-2.5V" symbol="VSS_VDD"/>
<gate name="P-SRAM2-2.5V" symbol="VSS_VDD"/>
<gate name="PWR16-2.5V" symbol="VSS_VDD"/>
<gate name="PWR17-2.5V" symbol="VSS_VDD"/>
<gate name="PWR18-2.5V" symbol="VSS_VDD"/>
<gate name="PWR19-2.5V" symbol="VSS_VDD"/>
<gate name="PWR20-2.5V" symbol="VSS_VDD"/>
<gate name="PWR21-2.5V" symbol="VSS_VDD"/>
<gate name="P-SC-5V" symbol="VSS_VDD"/>
<gate name="P-DM-5V" symbol="VSS_VDD"/>
<gate name="JTAG" symbol="JTAG-OCSD"/>
<gate name="A" symbol="TC1775"/>
<gate name="PWR22" symbol="VSS"/>
<gate name="PWR23" symbol="VSS"/>
<gate name="PWR24" symbol="VSS"/>
<gate name="PWR25" symbol="VSS"/>
<gate name="PWR26" symbol="VSS"/>
</gates>
<devices>
<device name="" package="P-BGA329">
<connects>
<connect gate="A" pin="BYPASS" pad="W22"/>
<connect gate="A" pin="CFG0" pad="Y23"/>
<connect gate="A" pin="CFG1" pad="Y22"/>
<connect gate="A" pin="CFG2" pad="W21"/>
<connect gate="A" pin="CFG3" pad="W23"/>
<connect gate="A" pin="CLKIN" pad="T1"/>
<connect gate="A" pin="CLKOUT" pad="R1"/>
<connect gate="A" pin="CLKSEL0" pad="V21"/>
<connect gate="A" pin="CLKSEL1" pad="V23"/>
<connect gate="A" pin="CLKSEL2" pad="V22"/>
<connect gate="A" pin="HDRST" pad="W20"/>
<connect gate="A" pin="NMI" pad="Y20"/>
<connect gate="A" pin="PORST" pad="Y21"/>
<connect gate="A" pin="TESTMODE" pad="AB23"/>
<connect gate="A" pin="VAGND@0" pad="B8"/>
<connect gate="A" pin="VAGND@1" pad="G4"/>
<connect gate="A" pin="VAREF@0" pad="C8"/>
<connect gate="A" pin="VAREF@1" pad="G2"/>
<connect gate="A" pin="VDD@0" pad="AC21"/>
<connect gate="A" pin="VDD@1" pad="AA22"/>
<connect gate="A" pin="VDDA@0" pad="D9"/>
<connect gate="A" pin="VDDA@1" pad="H1"/>
<connect gate="A" pin="VSS@0" pad="AA21"/>
<connect gate="A" pin="VSS@1" pad="AA23"/>
<connect gate="A" pin="VSSA@0" pad="A9"/>
<connect gate="A" pin="VSSA@1" pad="G3"/>
<connect gate="A" pin="XTAL1" pad="AC23"/>
<connect gate="A" pin="XTAL2" pad="AC22"/>
<connect gate="A" pin="XTAL3" pad="AB21"/>
<connect gate="A" pin="XTAL4" pad="AA20"/>
<connect gate="AD0-15" pin="0" pad="N1"/>
<connect gate="AD0-15" pin="1" pad="N4"/>
<connect gate="AD0-15" pin="10" pad="U3"/>
<connect gate="AD0-15" pin="11" pad="U2"/>
<connect gate="AD0-15" pin="12" pad="U4"/>
<connect gate="AD0-15" pin="13" pad="U1"/>
<connect gate="AD0-15" pin="14" pad="V2"/>
<connect gate="AD0-15" pin="15" pad="V1"/>
<connect gate="AD0-15" pin="2" pad="P3"/>
<connect gate="AD0-15" pin="3" pad="P2"/>
<connect gate="AD0-15" pin="4" pad="P1"/>
<connect gate="AD0-15" pin="5" pad="R3"/>
<connect gate="AD0-15" pin="6" pad="R2"/>
<connect gate="AD0-15" pin="7" pad="R4"/>
<connect gate="AD0-15" pin="8" pad="T3"/>
<connect gate="AD0-15" pin="9" pad="T2"/>
<connect gate="AD16-31" pin="0" pad="H2"/>
<connect gate="AD16-31" pin="1" pad="H3"/>
<connect gate="AD16-31" pin="10" pad="L3"/>
<connect gate="AD16-31" pin="11" pad="M3"/>
<connect gate="AD16-31" pin="12" pad="M1"/>
<connect gate="AD16-31" pin="13" pad="M2"/>
<connect gate="AD16-31" pin="14" pad="N2"/>
<connect gate="AD16-31" pin="15" pad="N3"/>
<connect gate="AD16-31" pin="2" pad="J1"/>
<connect gate="AD16-31" pin="3" pad="J4"/>
<connect gate="AD16-31" pin="4" pad="J2"/>
<connect gate="AD16-31" pin="5" pad="J3"/>
<connect gate="AD16-31" pin="6" pad="K1"/>
<connect gate="AD16-31" pin="7" pad="K2"/>
<connect gate="AD16-31" pin="8" pad="L1"/>
<connect gate="AD16-31" pin="9" pad="L2"/>
<connect gate="JTAG" pin="!BRKIN" pad="AC20"/>
<connect gate="JTAG" pin="!BRKOUT" pad="AC18"/>
<connect gate="JTAG" pin="!OCDSE" pad="Y19"/>
<connect gate="JTAG" pin="!TRST" pad="AA19"/>
<connect gate="JTAG" pin="TCK" pad="AB19"/>
<connect gate="JTAG" pin="TDI" pad="AC19"/>
<connect gate="JTAG" pin="TDO" pad="AA18"/>
<connect gate="JTAG" pin="TMS" pad="AB20"/>
<connect gate="NC" pin="NC@0" pad="AB15"/>
<connect gate="NC" pin="NC@1" pad="D10"/>
<connect gate="NC" pin="NC@2" pad="Y14"/>
<connect gate="NC" pin="NC@3" pad="AB22"/>
<connect gate="NC" pin="NC@4" pad="C14"/>
<connect gate="NC" pin="NC@5" pad="K3"/>
<connect gate="NC" pin="NC@6" pad="AC3"/>
<connect gate="NC" pin="NC@7" pad="L4"/>
<connect gate="NC" pin="NC@8" pad="D21"/>
<connect gate="NC" pin="NC@9" pad="Y16"/>
<connect gate="P-DM-5V" pin="VDD" pad="C3"/>
<connect gate="P-DM-5V" pin="VSS" pad="N12"/>
<connect gate="P-SB-2.5V" pin="VDD" pad="B14"/>
<connect gate="P-SB-2.5V" pin="VSS" pad="N13"/>
<connect gate="P-SC-5V" pin="VDD" pad="A1"/>
<connect gate="P-SC-5V" pin="VSS" pad="A2"/>
<connect gate="P-SRAM1-2.5V" pin="VDD" pad="AC17"/>
<connect gate="P-SRAM1-2.5V" pin="VSS" pad="N14"/>
<connect gate="P-SRAM2-2.5V" pin="VDD" pad="AB18"/>
<connect gate="P-SRAM2-2.5V" pin="VSS" pad="A3"/>
<connect gate="P2" pin="0" pad="AB3"/>
<connect gate="P2" pin="1" pad="AA4"/>
<connect gate="P2" pin="10" pad="AB6"/>
<connect gate="P2" pin="11" pad="AC7"/>
<connect gate="P2" pin="12" pad="Y7"/>
<connect gate="P2" pin="13" pad="AB7"/>
<connect gate="P2" pin="14" pad="AA7"/>
<connect gate="P2" pin="15" pad="AC8"/>
<connect gate="P2" pin="2" pad="Y5"/>
<connect gate="P2" pin="3" pad="AC4"/>
<connect gate="P2" pin="4" pad="AB4"/>
<connect gate="P2" pin="5" pad="AA5"/>
<connect gate="P2" pin="6" pad="AC5"/>
<connect gate="P2" pin="7" pad="AB5"/>
<connect gate="P2" pin="8" pad="AA6"/>
<connect gate="P2" pin="9" pad="AC6"/>
<connect gate="P3" pin="0" pad="AB8"/>
<connect gate="P3" pin="1" pad="AA8"/>
<connect gate="P3" pin="10" pad="AC11"/>
<connect gate="P3" pin="11" pad="AB11"/>
<connect gate="P3" pin="12" pad="AA11"/>
<connect gate="P3" pin="13" pad="AA12"/>
<connect gate="P3" pin="14" pad="AC12"/>
<connect gate="P3" pin="15" pad="AB12"/>
<connect gate="P3" pin="2" pad="AC9"/>
<connect gate="P3" pin="3" pad="Y9"/>
<connect gate="P3" pin="4" pad="AB9"/>
<connect gate="P3" pin="5" pad="AA9"/>
<connect gate="P3" pin="6" pad="AC10"/>
<connect gate="P3" pin="7" pad="AB10"/>
<connect gate="P3" pin="8" pad="AA10"/>
<connect gate="P3" pin="9" pad="Y11"/>
<connect gate="P4" pin="0" pad="V3"/>
<connect gate="P4" pin="1" pad="W2"/>
<connect gate="P4" pin="10" pad="AA3"/>
<connect gate="P4" pin="11" pad="AB1"/>
<connect gate="P4" pin="12" pad="AC1"/>
<connect gate="P4" pin="13" pad="AC2"/>
<connect gate="P4" pin="14" pad="AB2"/>
<connect gate="P4" pin="15" pad="Y4"/>
<connect gate="P4" pin="2" pad="W1"/>
<connect gate="P4" pin="3" pad="W3"/>
<connect gate="P4" pin="4" pad="Y2"/>
<connect gate="P4" pin="5" pad="Y1"/>
<connect gate="P4" pin="6" pad="W4"/>
<connect gate="P4" pin="7" pad="Y3"/>
<connect gate="P4" pin="8" pad="AA2"/>
<connect gate="P4" pin="9" pad="AA1"/>
<connect gate="P5/TRACE" pin="0" pad="AB13"/>
<connect gate="P5/TRACE" pin="1" pad="AA13"/>
<connect gate="P5/TRACE" pin="10" pad="AA16"/>
<connect gate="P5/TRACE" pin="11" pad="AB16"/>
<connect gate="P5/TRACE" pin="12" pad="AC16"/>
<connect gate="P5/TRACE" pin="13" pad="AA17"/>
<connect gate="P5/TRACE" pin="14" pad="AB17"/>
<connect gate="P5/TRACE" pin="15" pad="Y17"/>
<connect gate="P5/TRACE" pin="2" pad="AC13"/>
<connect gate="P5/TRACE" pin="3" pad="Y13"/>
<connect gate="P5/TRACE" pin="4" pad="AA14"/>
<connect gate="P5/TRACE" pin="5" pad="AB14"/>
<connect gate="P5/TRACE" pin="6" pad="AC14"/>
<connect gate="P5/TRACE" pin="7" pad="AA15"/>
<connect gate="P5/TRACE" pin="8" pad="Y15"/>
<connect gate="P5/TRACE" pin="9" pad="AC15"/>
<connect gate="P6/ADC0" pin="0" pad="B3"/>
<connect gate="P6/ADC0" pin="1" pad="C4"/>
<connect gate="P6/ADC0" pin="10" pad="B6"/>
<connect gate="P6/ADC0" pin="11" pad="A7"/>
<connect gate="P6/ADC0" pin="12" pad="D7"/>
<connect gate="P6/ADC0" pin="13" pad="B7"/>
<connect gate="P6/ADC0" pin="14" pad="C7"/>
<connect gate="P6/ADC0" pin="15" pad="A8"/>
<connect gate="P6/ADC0" pin="2" pad="D5"/>
<connect gate="P6/ADC0" pin="3" pad="A4"/>
<connect gate="P6/ADC0" pin="4" pad="B4"/>
<connect gate="P6/ADC0" pin="5" pad="C5"/>
<connect gate="P6/ADC0" pin="6" pad="A5"/>
<connect gate="P6/ADC0" pin="7" pad="B5"/>
<connect gate="P6/ADC0" pin="8" pad="C6"/>
<connect gate="P6/ADC0" pin="9" pad="A6"/>
<connect gate="P7/ADC1" pin="0" pad="B1"/>
<connect gate="P7/ADC1" pin="1" pad="B2"/>
<connect gate="P7/ADC1" pin="10" pad="E1"/>
<connect gate="P7/ADC1" pin="11" pad="E2"/>
<connect gate="P7/ADC1" pin="12" pad="F3"/>
<connect gate="P7/ADC1" pin="13" pad="F1"/>
<connect gate="P7/ADC1" pin="14" pad="F2"/>
<connect gate="P7/ADC1" pin="15" pad="G1"/>
<connect gate="P7/ADC1" pin="2" pad="D4"/>
<connect gate="P7/ADC1" pin="3" pad="C1"/>
<connect gate="P7/ADC1" pin="4" pad="C2"/>
<connect gate="P7/ADC1" pin="5" pad="D3"/>
<connect gate="P7/ADC1" pin="6" pad="E4"/>
<connect gate="P7/ADC1" pin="7" pad="D1"/>
<connect gate="P7/ADC1" pin="8" pad="D2"/>
<connect gate="P7/ADC1" pin="9" pad="E3"/>
<connect gate="P8/GPTA" pin="0" pad="U23"/>
<connect gate="P8/GPTA" pin="1" pad="U20"/>
<connect gate="P8/GPTA" pin="10" pad="R21"/>
<connect gate="P8/GPTA" pin="11" pad="P23"/>
<connect gate="P8/GPTA" pin="12" pad="P22"/>
<connect gate="P8/GPTA" pin="13" pad="P21"/>
<connect gate="P8/GPTA" pin="14" pad="N20"/>
<connect gate="P8/GPTA" pin="15" pad="N23"/>
<connect gate="P8/GPTA" pin="2" pad="U22"/>
<connect gate="P8/GPTA" pin="3" pad="U21"/>
<connect gate="P8/GPTA" pin="4" pad="T23"/>
<connect gate="P8/GPTA" pin="5" pad="T22"/>
<connect gate="P8/GPTA" pin="6" pad="T21"/>
<connect gate="P8/GPTA" pin="7" pad="R23"/>
<connect gate="P8/GPTA" pin="8" pad="R20"/>
<connect gate="P8/GPTA" pin="9" pad="R22"/>
<connect gate="P9/GPTA" pin="0" pad="N22"/>
<connect gate="P9/GPTA" pin="1" pad="N21"/>
<connect gate="P9/GPTA" pin="10" pad="K22"/>
<connect gate="P9/GPTA" pin="11" pad="K23"/>
<connect gate="P9/GPTA" pin="12" pad="J21"/>
<connect gate="P9/GPTA" pin="13" pad="J22"/>
<connect gate="P9/GPTA" pin="14" pad="J20"/>
<connect gate="P9/GPTA" pin="15" pad="J23"/>
<connect gate="P9/GPTA" pin="2" pad="M21"/>
<connect gate="P9/GPTA" pin="3" pad="M23"/>
<connect gate="P9/GPTA" pin="4" pad="M22"/>
<connect gate="P9/GPTA" pin="5" pad="L22"/>
<connect gate="P9/GPTA" pin="6" pad="L21"/>
<connect gate="P9/GPTA" pin="7" pad="L23"/>
<connect gate="P9/GPTA" pin="8" pad="L20"/>
<connect gate="P9/GPTA" pin="9" pad="K21"/>
<connect gate="PORT10" pin="0" pad="H21"/>
<connect gate="PORT10" pin="1" pad="H22"/>
<connect gate="PORT10" pin="10" pad="E22"/>
<connect gate="PORT10" pin="11" pad="E23"/>
<connect gate="PORT10" pin="12" pad="E21"/>
<connect gate="PORT10" pin="13" pad="D22"/>
<connect gate="PORT10" pin="14" pad="D23"/>
<connect gate="PORT10" pin="15" pad="E20"/>
<connect gate="PORT10" pin="2" pad="H23"/>
<connect gate="PORT10" pin="3" pad="G21"/>
<connect gate="PORT10" pin="4" pad="G22"/>
<connect gate="PORT10" pin="5" pad="G20"/>
<connect gate="PORT10" pin="6" pad="G23"/>
<connect gate="PORT10" pin="7" pad="F22"/>
<connect gate="PORT10" pin="8" pad="F23"/>
<connect gate="PORT10" pin="9" pad="F21"/>
<connect gate="PORT11" pin="0" pad="C22"/>
<connect gate="PORT11" pin="1" pad="C23"/>
<connect gate="PORT11" pin="10" pad="C20"/>
<connect gate="PORT11" pin="11" pad="D19"/>
<connect gate="PORT11" pin="12" pad="A20"/>
<connect gate="PORT11" pin="13" pad="B20"/>
<connect gate="PORT11" pin="14" pad="C19"/>
<connect gate="PORT11" pin="15" pad="A19"/>
<connect gate="PORT11" pin="2" pad="C21"/>
<connect gate="PORT11" pin="3" pad="B23"/>
<connect gate="PORT11" pin="4" pad="A23"/>
<connect gate="PORT11" pin="5" pad="A22"/>
<connect gate="PORT11" pin="6" pad="B22"/>
<connect gate="PORT11" pin="7" pad="D20"/>
<connect gate="PORT11" pin="8" pad="A21"/>
<connect gate="PORT11" pin="9" pad="B21"/>
<connect gate="PORT12" pin="0" pad="D13"/>
<connect gate="PORT12" pin="1" pad="A13"/>
<connect gate="PORT12" pin="10" pad="D11"/>
<connect gate="PORT12" pin="11" pad="C10"/>
<connect gate="PORT12" pin="12" pad="B10"/>
<connect gate="PORT12" pin="13" pad="A10"/>
<connect gate="PORT12" pin="14" pad="C9"/>
<connect gate="PORT12" pin="15" pad="B9"/>
<connect gate="PORT12" pin="2" pad="B13"/>
<connect gate="PORT12" pin="3" pad="C13"/>
<connect gate="PORT12" pin="4" pad="C12"/>
<connect gate="PORT12" pin="5" pad="A12"/>
<connect gate="PORT12" pin="6" pad="B12"/>
<connect gate="PORT12" pin="7" pad="B11"/>
<connect gate="PORT12" pin="8" pad="C11"/>
<connect gate="PORT12" pin="9" pad="A11"/>
<connect gate="PORT13" pin="0" pad="B19"/>
<connect gate="PORT13" pin="1" pad="C18"/>
<connect gate="PORT13" pin="10" pad="C16"/>
<connect gate="PORT13" pin="11" pad="A15"/>
<connect gate="PORT13" pin="12" pad="D15"/>
<connect gate="PORT13" pin="13" pad="B15"/>
<connect gate="PORT13" pin="14" pad="C15"/>
<connect gate="PORT13" pin="15" pad="A14"/>
<connect gate="PORT13" pin="2" pad="A18"/>
<connect gate="PORT13" pin="3" pad="B18"/>
<connect gate="PORT13" pin="4" pad="A17"/>
<connect gate="PORT13" pin="5" pad="D17"/>
<connect gate="PORT13" pin="6" pad="B17"/>
<connect gate="PORT13" pin="7" pad="C17"/>
<connect gate="PORT13" pin="8" pad="A16"/>
<connect gate="PORT13" pin="9" pad="B16"/>
<connect gate="PWR1-2.5V" pin="VDD" pad="H4"/>
<connect gate="PWR1-2.5V" pin="VSS" pad="F4"/>
<connect gate="PWR10-3.3V" pin="VDD" pad="M20"/>
<connect gate="PWR10-3.3V" pin="VSS" pad="L10"/>
<connect gate="PWR11-3.3V" pin="VDD" pad="T20"/>
<connect gate="PWR11-3.3V" pin="VSS" pad="L11"/>
<connect gate="PWR12-2.5V" pin="VDD" pad="K4"/>
<connect gate="PWR12-2.5V" pin="VSS" pad="L12"/>
<connect gate="PWR13-2.5V" pin="VDD" pad="P4"/>
<connect gate="PWR13-2.5V" pin="VSS" pad="L13"/>
<connect gate="PWR14-2.5V" pin="VDD" pad="V4"/>
<connect gate="PWR14-2.5V" pin="VSS" pad="L14"/>
<connect gate="PWR15-2.5V" pin="VDD" pad="D6"/>
<connect gate="PWR15-2.5V" pin="VSS" pad="P10"/>
<connect gate="PWR16-2.5V" pin="VDD" pad="D14"/>
<connect gate="PWR16-2.5V" pin="VSS" pad="M10"/>
<connect gate="PWR17-2.5V" pin="VDD" pad="Y10"/>
<connect gate="PWR17-2.5V" pin="VSS" pad="M11"/>
<connect gate="PWR18-2.5V" pin="VDD" pad="Y18"/>
<connect gate="PWR18-2.5V" pin="VSS" pad="M12"/>
<connect gate="PWR19-2.5V" pin="VDD" pad="F20"/>
<connect gate="PWR19-2.5V" pin="VSS" pad="M13"/>
<connect gate="PWR2-2.5V" pin="VDD" pad="M4"/>
<connect gate="PWR2-2.5V" pin="VSS" pad="Y6"/>
<connect gate="PWR20-2.5V" pin="VDD" pad="K20"/>
<connect gate="PWR20-2.5V" pin="VSS" pad="M14"/>
<connect gate="PWR21-2.5V" pin="VDD" pad="P20"/>
<connect gate="PWR21-2.5V" pin="VSS" pad="P13"/>
<connect gate="PWR22" pin="VSS" pad="P11"/>
<connect gate="PWR23" pin="VSS" pad="P12"/>
<connect gate="PWR24" pin="VSS" pad="P14"/>
<connect gate="PWR25" pin="VSS" pad="N10"/>
<connect gate="PWR26" pin="VSS" pad="N11"/>
<connect gate="PWR3-2.5V" pin="VDD" pad="T4"/>
<connect gate="PWR3-2.5V" pin="VSS" pad="V20"/>
<connect gate="PWR4-2.5V" pin="VDD" pad="Y8"/>
<connect gate="PWR4-2.5V" pin="VSS" pad="D18"/>
<connect gate="PWR5-2.5V" pin="VDD" pad="Y12"/>
<connect gate="PWR5-2.5V" pin="VSS" pad="K10"/>
<connect gate="PWR6-3.3V" pin="VDD" pad="D8"/>
<connect gate="PWR6-3.3V" pin="VSS" pad="K11"/>
<connect gate="PWR7-3.3V" pin="VDD" pad="D12"/>
<connect gate="PWR7-3.3V" pin="VSS" pad="K12"/>
<connect gate="PWR8-3.3V" pin="VDD" pad="D16"/>
<connect gate="PWR8-3.3V" pin="VSS" pad="K13"/>
<connect gate="PWR9-3.3V" pin="VDD" pad="H20"/>
<connect gate="PWR9-3.3V" pin="VSS" pad="K14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1765" prefix="IC">
<description>&lt;b&gt;TC1765 (AUDO1)&lt;/b&gt; 32-bit microcontroller&lt;p&gt;
for automotive and industrial applications &lt;br&gt;
(e.g. engine management, transmission, starter generator or 3-phase motor control)&lt;br&gt;
Source: http://www.infineon.com ..</description>
<gates>
<gate name="TP" symbol="PORT16"/>
<gate name="D" symbol="D31"/>
<gate name="A" symbol="A23"/>
<gate name="AN" symbol="AN23"/>
<gate name="JTAG" symbol="JTAG-OCSD"/>
<gate name="P1" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="P3" symbol="PORT16"/>
<gate name="P0" symbol="PORT16"/>
<gate name="PW1" symbol="VSS_VDD"/>
<gate name="PW2" symbol="VSS_VDD"/>
<gate name="PW3" symbol="VSS_VDD"/>
<gate name="PW4" symbol="VSS_VDD"/>
<gate name="PW5" symbol="VSS_VDD"/>
<gate name="PW6" symbol="VSS_VDD"/>
<gate name="PW7" symbol="VSS_VDD"/>
<gate name="PW8" symbol="VSS_VDD"/>
<gate name="PW9" symbol="VSS_VDD"/>
<gate name="PW10" symbol="VSS_VDD"/>
<gate name="G" symbol="TC1765"/>
<gate name="AREF0" symbol="VSS_VDD"/>
<gate name="AREF1" symbol="VSS_VDD"/>
<gate name="PW11" symbol="VSS_VDD"/>
<gate name="PW12" symbol="VSS_VDD"/>
<gate name="PW13" symbol="VSS_VDD"/>
<gate name="PW14" symbol="VSS_VDD"/>
<gate name="PW15" symbol="VSS_VDD"/>
<gate name="PW16" symbol="VSS_VDD"/>
<gate name="PW17" symbol="VSS_VDD"/>
<gate name="PW18" symbol="VSS_VDD"/>
<gate name="PW19" symbol="VSS_VDD"/>
<gate name="PW20" symbol="VSS_VDD"/>
<gate name="PW21" symbol="VSS_VDD"/>
<gate name="PW23" symbol="GND6"/>
</gates>
<devices>
<device name="" package="P-LBGA-260">
<connects>
<connect gate="A" pin="A0" pad="T5"/>
<connect gate="A" pin="A1" pad="V4"/>
<connect gate="A" pin="A10" pad="U7"/>
<connect gate="A" pin="A11" pad="T7"/>
<connect gate="A" pin="A12" pad="V8"/>
<connect gate="A" pin="A13" pad="U14"/>
<connect gate="A" pin="A14" pad="U8"/>
<connect gate="A" pin="A15" pad="T8"/>
<connect gate="A" pin="A16" pad="T9"/>
<connect gate="A" pin="A17" pad="V14"/>
<connect gate="A" pin="A18" pad="U9"/>
<connect gate="A" pin="A19" pad="R9"/>
<connect gate="A" pin="A2" pad="U5"/>
<connect gate="A" pin="A20" pad="V13"/>
<connect gate="A" pin="A21" pad="T11"/>
<connect gate="A" pin="A22" pad="V10"/>
<connect gate="A" pin="A23" pad="U10"/>
<connect gate="A" pin="A3" pad="R6"/>
<connect gate="A" pin="A4" pad="V5"/>
<connect gate="A" pin="A5" pad="R7"/>
<connect gate="A" pin="A6" pad="T6"/>
<connect gate="A" pin="A7" pad="U6"/>
<connect gate="A" pin="A8" pad="R8"/>
<connect gate="A" pin="A9" pad="V6"/>
<connect gate="AN" pin="AN0" pad="A7"/>
<connect gate="AN" pin="AN1" pad="D6"/>
<connect gate="AN" pin="AN10" pad="C3"/>
<connect gate="AN" pin="AN11" pad="B3"/>
<connect gate="AN" pin="AN12" pad="D3"/>
<connect gate="AN" pin="AN13" pad="D4"/>
<connect gate="AN" pin="AN14" pad="E4"/>
<connect gate="AN" pin="AN15" pad="E3"/>
<connect gate="AN" pin="AN16" pad="A2"/>
<connect gate="AN" pin="AN17" pad="A1"/>
<connect gate="AN" pin="AN18" pad="B2"/>
<connect gate="AN" pin="AN19" pad="B1"/>
<connect gate="AN" pin="AN2" pad="B6"/>
<connect gate="AN" pin="AN20" pad="C2"/>
<connect gate="AN" pin="AN21" pad="F4"/>
<connect gate="AN" pin="AN22" pad="F3"/>
<connect gate="AN" pin="AN23" pad="D2"/>
<connect gate="AN" pin="AN3" pad="D5"/>
<connect gate="AN" pin="AN4" pad="A6"/>
<connect gate="AN" pin="AN5" pad="B5"/>
<connect gate="AN" pin="AN6" pad="C5"/>
<connect gate="AN" pin="AN7" pad="A5"/>
<connect gate="AN" pin="AN8" pad="A3"/>
<connect gate="AN" pin="AN9" pad="C4"/>
<connect gate="AREF0" pin="VDD" pad="C1"/>
<connect gate="AREF0" pin="VSS" pad="E2"/>
<connect gate="AREF1" pin="VDD" pad="A8"/>
<connect gate="AREF1" pin="VSS" pad="C6"/>
<connect gate="D" pin="D0" pad="T3"/>
<connect gate="D" pin="D1" pad="R4"/>
<connect gate="D" pin="D10" pad="L4"/>
<connect gate="D" pin="D11" pad="M3"/>
<connect gate="D" pin="D12" pad="N2"/>
<connect gate="D" pin="D13" pad="M2"/>
<connect gate="D" pin="D14" pad="L3"/>
<connect gate="D" pin="D15" pad="M1"/>
<connect gate="D" pin="D16" pad="L1"/>
<connect gate="D" pin="D17" pad="K1"/>
<connect gate="D" pin="D18" pad="K2"/>
<connect gate="D" pin="D19" pad="K3"/>
<connect gate="D" pin="D2" pad="P4"/>
<connect gate="D" pin="D20" pad="J1"/>
<connect gate="D" pin="D21" pad="J2"/>
<connect gate="D" pin="D22" pad="H2"/>
<connect gate="D" pin="D23" pad="H1"/>
<connect gate="D" pin="D24" pad="J4"/>
<connect gate="D" pin="D25" pad="H3"/>
<connect gate="D" pin="D26" pad="G2"/>
<connect gate="D" pin="D27" pad="G1"/>
<connect gate="D" pin="D28" pad="F1"/>
<connect gate="D" pin="D29" pad="E1"/>
<connect gate="D" pin="D3" pad="R2"/>
<connect gate="D" pin="D30" pad="F2"/>
<connect gate="D" pin="D31" pad="H4"/>
<connect gate="D" pin="D4" pad="R1"/>
<connect gate="D" pin="D5" pad="R3"/>
<connect gate="D" pin="D6" pad="N4"/>
<connect gate="D" pin="D7" pad="P3"/>
<connect gate="D" pin="D8" pad="M4"/>
<connect gate="D" pin="D9" pad="N3"/>
<connect gate="G" pin="/BAA" pad="U4"/>
<connect gate="G" pin="/BC0" pad="U2"/>
<connect gate="G" pin="/BC1" pad="V1"/>
<connect gate="G" pin="/BC2" pad="U3"/>
<connect gate="G" pin="/BC3" pad="V2"/>
<connect gate="G" pin="/CDEMU/!CSOVK" pad="V11"/>
<connect gate="G" pin="/CODE" pad="V3"/>
<connect gate="G" pin="/CS0" pad="U12"/>
<connect gate="G" pin="/CS1" pad="V12"/>
<connect gate="G" pin="/CS2" pad="T10"/>
<connect gate="G" pin="/CS3" pad="R10"/>
<connect gate="G" pin="/HDRST" pad="P18"/>
<connect gate="G" pin="/NMI" pad="U17"/>
<connect gate="G" pin="/PO_RST" pad="T17"/>
<connect gate="G" pin="/TEST/MODE" pad="V16"/>
<connect gate="G" pin="/WAIT/!IND" pad="R5"/>
<connect gate="G" pin="ADV" pad="U1"/>
<connect gate="G" pin="BYPASS" pad="N17"/>
<connect gate="G" pin="CPUCLK" pad="R13"/>
<connect gate="G" pin="ECIN" pad="N1"/>
<connect gate="G" pin="ECOUT" pad="P1"/>
<connect gate="G" pin="NC@0" pad="V17"/>
<connect gate="G" pin="NC@1" pad="V18"/>
<connect gate="G" pin="P4.0" pad="D14"/>
<connect gate="G" pin="P4.1" pad="C13"/>
<connect gate="G" pin="P4.2" pad="A17"/>
<connect gate="G" pin="P4.3" pad="B15"/>
<connect gate="G" pin="P4.4" pad="C16"/>
<connect gate="G" pin="P4.5" pad="D13"/>
<connect gate="G" pin="P4.6" pad="C15"/>
<connect gate="G" pin="P4.7" pad="C12"/>
<connect gate="G" pin="P5.0" pad="D12"/>
<connect gate="G" pin="P5.1" pad="B13"/>
<connect gate="G" pin="P5.2" pad="B14"/>
<connect gate="G" pin="P5.3" pad="C11"/>
<connect gate="G" pin="P5.4" pad="A16"/>
<connect gate="G" pin="RD" pad="T1"/>
<connect gate="G" pin="RD/!WR" pad="T2"/>
<connect gate="G" pin="XTAL1" pad="U18"/>
<connect gate="G" pin="XTAL2" pad="T18"/>
<connect gate="JTAG" pin="!BRKIN" pad="U15"/>
<connect gate="JTAG" pin="!BRKOUT" pad="T12"/>
<connect gate="JTAG" pin="!OCDSE" pad="R11"/>
<connect gate="JTAG" pin="!TRST" pad="R14"/>
<connect gate="JTAG" pin="TCK" pad="T13"/>
<connect gate="JTAG" pin="TDI" pad="T14"/>
<connect gate="JTAG" pin="TDO" pad="R12"/>
<connect gate="JTAG" pin="TMS" pad="V15"/>
<connect gate="P0" pin="0" pad="A10"/>
<connect gate="P0" pin="1" pad="D7"/>
<connect gate="P0" pin="10" pad="A14"/>
<connect gate="P0" pin="11" pad="C9"/>
<connect gate="P0" pin="12" pad="C10"/>
<connect gate="P0" pin="13" pad="D10"/>
<connect gate="P0" pin="14" pad="A15"/>
<connect gate="P0" pin="15" pad="B11"/>
<connect gate="P0" pin="2" pad="B8"/>
<connect gate="P0" pin="3" pad="C7"/>
<connect gate="P0" pin="4" pad="A11"/>
<connect gate="P0" pin="5" pad="A12"/>
<connect gate="P0" pin="6" pad="D8"/>
<connect gate="P0" pin="7" pad="B9"/>
<connect gate="P0" pin="8" pad="A13"/>
<connect gate="P0" pin="9" pad="B10"/>
<connect gate="P1" pin="0" pad="N18"/>
<connect gate="P1" pin="1" pad="R16"/>
<connect gate="P1" pin="10" pad="M16"/>
<connect gate="P1" pin="11" pad="L16"/>
<connect gate="P1" pin="12" pad="K17"/>
<connect gate="P1" pin="13" pad="K18"/>
<connect gate="P1" pin="14" pad="L15"/>
<connect gate="P1" pin="15" pad="K16"/>
<connect gate="P1" pin="2" pad="R15"/>
<connect gate="P1" pin="3" pad="M17"/>
<connect gate="P1" pin="4" pad="N16"/>
<connect gate="P1" pin="5" pad="P15"/>
<connect gate="P1" pin="6" pad="M18"/>
<connect gate="P1" pin="7" pad="L18"/>
<connect gate="P1" pin="8" pad="P16"/>
<connect gate="P1" pin="9" pad="U16"/>
<connect gate="P2" pin="0" pad="J18"/>
<connect gate="P2" pin="1" pad="T15"/>
<connect gate="P2" pin="10" pad="G18"/>
<connect gate="P2" pin="11" pad="H15"/>
<connect gate="P2" pin="12" pad="G15"/>
<connect gate="P2" pin="13" pad="G17"/>
<connect gate="P2" pin="14" pad="G16"/>
<connect gate="P2" pin="15" pad="F18"/>
<connect gate="P2" pin="2" pad="N15"/>
<connect gate="P2" pin="3" pad="J17"/>
<connect gate="P2" pin="4" pad="H18"/>
<connect gate="P2" pin="5" pad="J16"/>
<connect gate="P2" pin="6" pad="T16"/>
<connect gate="P2" pin="7" pad="M15"/>
<connect gate="P2" pin="8" pad="J15"/>
<connect gate="P2" pin="9" pad="H16"/>
<connect gate="P3" pin="0" pad="F16"/>
<connect gate="P3" pin="1" pad="F15"/>
<connect gate="P3" pin="10" pad="B18"/>
<connect gate="P3" pin="11" pad="A18"/>
<connect gate="P3" pin="12" pad="C14"/>
<connect gate="P3" pin="13" pad="D15"/>
<connect gate="P3" pin="14" pad="B17"/>
<connect gate="P3" pin="15" pad="B16"/>
<connect gate="P3" pin="2" pad="E18"/>
<connect gate="P3" pin="3" pad="E16"/>
<connect gate="P3" pin="4" pad="E15"/>
<connect gate="P3" pin="5" pad="E17"/>
<connect gate="P3" pin="6" pad="D18"/>
<connect gate="P3" pin="7" pad="D17"/>
<connect gate="P3" pin="8" pad="C18"/>
<connect gate="P3" pin="9" pad="C17"/>
<connect gate="PW1" pin="VDD" pad="J3"/>
<connect gate="PW1" pin="VSS" pad="K4"/>
<connect gate="PW10" pin="VDD" pad="C8"/>
<connect gate="PW10" pin="VSS" pad="J11"/>
<connect gate="PW11" pin="VDD" pad="A9"/>
<connect gate="PW11" pin="VSS" pad="A4"/>
<connect gate="PW12" pin="VDD" pad="B4"/>
<connect gate="PW12" pin="VSS" pad="B7"/>
<connect gate="PW13" pin="VDD" pad="B12"/>
<connect gate="PW13" pin="VSS" pad="D1"/>
<connect gate="PW14" pin="VDD" pad="D11"/>
<connect gate="PW14" pin="VSS" pad="D9"/>
<connect gate="PW15" pin="VDD" pad="D16"/>
<connect gate="PW15" pin="VSS" pad="J12"/>
<connect gate="PW16" pin="VDD" pad="G3"/>
<connect gate="PW16" pin="VSS" pad="K7"/>
<connect gate="PW17" pin="VDD" pad="G4"/>
<connect gate="PW17" pin="VSS" pad="K8"/>
<connect gate="PW18" pin="VDD" pad="H17"/>
<connect gate="PW18" pin="VSS" pad="K9"/>
<connect gate="PW19" pin="VDD" pad="R18"/>
<connect gate="PW19" pin="VSS" pad="K10"/>
<connect gate="PW2" pin="VDD" pad="L2"/>
<connect gate="PW2" pin="VSS" pad="G9"/>
<connect gate="PW20" pin="VDD" pad="P17"/>
<connect gate="PW20" pin="VSS" pad="K11"/>
<connect gate="PW21" pin="VDD" pad="L17"/>
<connect gate="PW21" pin="VSS" pad="K12"/>
<connect gate="PW23" pin="GND@0" pad="K15"/>
<connect gate="PW23" pin="GND@1" pad="L9"/>
<connect gate="PW23" pin="GND@2" pad="L10"/>
<connect gate="PW23" pin="GND@3" pad="M9"/>
<connect gate="PW23" pin="GND@4" pad="M10"/>
<connect gate="PW23" pin="GND@5" pad="R17"/>
<connect gate="PW3" pin="VDD" pad="P2"/>
<connect gate="PW3" pin="VSS" pad="G10"/>
<connect gate="PW4" pin="VDD" pad="T4"/>
<connect gate="PW4" pin="VSS" pad="H9"/>
<connect gate="PW5" pin="VDD" pad="V7"/>
<connect gate="PW5" pin="VSS" pad="H10"/>
<connect gate="PW6" pin="VDD" pad="V9"/>
<connect gate="PW6" pin="VSS" pad="J7"/>
<connect gate="PW7" pin="VDD" pad="U11"/>
<connect gate="PW7" pin="VSS" pad="J8"/>
<connect gate="PW8" pin="VDD" pad="U13"/>
<connect gate="PW8" pin="VSS" pad="J9"/>
<connect gate="PW9" pin="VDD" pad="F17"/>
<connect gate="PW9" pin="VSS" pad="J10"/>
<connect gate="TP" pin="0" pad="G7"/>
<connect gate="TP" pin="1" pad="G8"/>
<connect gate="TP" pin="10" pad="L11"/>
<connect gate="TP" pin="11" pad="L12"/>
<connect gate="TP" pin="12" pad="H11"/>
<connect gate="TP" pin="13" pad="H12"/>
<connect gate="TP" pin="14" pad="G11"/>
<connect gate="TP" pin="15" pad="G12"/>
<connect gate="TP" pin="2" pad="H7"/>
<connect gate="TP" pin="3" pad="H8"/>
<connect gate="TP" pin="4" pad="L7"/>
<connect gate="TP" pin="5" pad="L8"/>
<connect gate="TP" pin="6" pad="M7"/>
<connect gate="TP" pin="7" pad="M8"/>
<connect gate="TP" pin="8" pad="M11"/>
<connect gate="TP" pin="9" pad="M12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1920" prefix="IC">
<description>&lt;b&gt;32bit Single Chip Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. TC1920_umsu_V12.pdf</description>
<gates>
<gate name="DEBUG" symbol="JTAG-OCSD"/>
<gate name="P3" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="AD" symbol="D31"/>
<gate name="P1" symbol="PORT8"/>
<gate name="P0" symbol="PORT8"/>
<gate name="EBU" symbol="A23"/>
<gate name="P5/TRACE" symbol="PORT16"/>
<gate name="PWR" symbol="TC1920PWR"/>
<gate name="PWR2" symbol="TC1920PWR2"/>
<gate name="G" symbol="TC1920"/>
</gates>
<devices>
<device name="" package="P-LBGA-260">
<connects>
<connect gate="AD" pin="D0" pad="L3"/>
<connect gate="AD" pin="D1" pad="L2"/>
<connect gate="AD" pin="D10" pad="H1"/>
<connect gate="AD" pin="D11" pad="H2"/>
<connect gate="AD" pin="D12" pad="H3"/>
<connect gate="AD" pin="D13" pad="G1"/>
<connect gate="AD" pin="D14" pad="G2"/>
<connect gate="AD" pin="D15" pad="G3"/>
<connect gate="AD" pin="D16" pad="H4"/>
<connect gate="AD" pin="D17" pad="G4"/>
<connect gate="AD" pin="D18" pad="E4"/>
<connect gate="AD" pin="D19" pad="F1"/>
<connect gate="AD" pin="D2" pad="K3"/>
<connect gate="AD" pin="D20" pad="F2"/>
<connect gate="AD" pin="D21" pad="F4"/>
<connect gate="AD" pin="D22" pad="F3"/>
<connect gate="AD" pin="D23" pad="E1"/>
<connect gate="AD" pin="D24" pad="E2"/>
<connect gate="AD" pin="D25" pad="E3"/>
<connect gate="AD" pin="D26" pad="D1"/>
<connect gate="AD" pin="D27" pad="C1"/>
<connect gate="AD" pin="D28" pad="D2"/>
<connect gate="AD" pin="D29" pad="D3"/>
<connect gate="AD" pin="D3" pad="K4"/>
<connect gate="AD" pin="D30" pad="C2"/>
<connect gate="AD" pin="D31" pad="B1"/>
<connect gate="AD" pin="D4" pad="L1"/>
<connect gate="AD" pin="D5" pad="K2"/>
<connect gate="AD" pin="D6" pad="K1"/>
<connect gate="AD" pin="D7" pad="J3"/>
<connect gate="AD" pin="D8" pad="J1"/>
<connect gate="AD" pin="D9" pad="J2"/>
<connect gate="DEBUG" pin="!BRKIN" pad="U15"/>
<connect gate="DEBUG" pin="!BRKOUT" pad="T14"/>
<connect gate="DEBUG" pin="!OCDSE" pad="V16"/>
<connect gate="DEBUG" pin="!TRST" pad="U17"/>
<connect gate="DEBUG" pin="TCK" pad="T16"/>
<connect gate="DEBUG" pin="TDI" pad="V17"/>
<connect gate="DEBUG" pin="TDO" pad="U16"/>
<connect gate="DEBUG" pin="TMS" pad="T15"/>
<connect gate="EBU" pin="A0" pad="V2"/>
<connect gate="EBU" pin="A1" pad="T5"/>
<connect gate="EBU" pin="A10" pad="T1"/>
<connect gate="EBU" pin="A11" pad="P3"/>
<connect gate="EBU" pin="A12" pad="R5"/>
<connect gate="EBU" pin="A13" pad="R2"/>
<connect gate="EBU" pin="A14" pad="P2"/>
<connect gate="EBU" pin="A15" pad="N3"/>
<connect gate="EBU" pin="A16" pad="R1"/>
<connect gate="EBU" pin="A17" pad="P1"/>
<connect gate="EBU" pin="A18" pad="N2"/>
<connect gate="EBU" pin="A19" pad="P4"/>
<connect gate="EBU" pin="A2" pad="V1"/>
<connect gate="EBU" pin="A20" pad="M3"/>
<connect gate="EBU" pin="A21" pad="N4"/>
<connect gate="EBU" pin="A22" pad="M4"/>
<connect gate="EBU" pin="A23" pad="N1"/>
<connect gate="EBU" pin="A3" pad="U3"/>
<connect gate="EBU" pin="A4" pad="T4"/>
<connect gate="EBU" pin="A5" pad="U2"/>
<connect gate="EBU" pin="A6" pad="T3"/>
<connect gate="EBU" pin="A7" pad="U1"/>
<connect gate="EBU" pin="A8" pad="R3"/>
<connect gate="EBU" pin="A9" pad="T2"/>
<connect gate="G" pin="/ADV" pad="R10"/>
<connect gate="G" pin="/BAA" pad="U8"/>
<connect gate="G" pin="/BC0" pad="T7"/>
<connect gate="G" pin="/BC1" pad="R6"/>
<connect gate="G" pin="/BC2" pad="V4"/>
<connect gate="G" pin="/BC3" pad="U6"/>
<connect gate="G" pin="/CAS" pad="T6"/>
<connect gate="G" pin="/CMDELAY" pad="V9"/>
<connect gate="G" pin="/CSGLB" pad="U9"/>
<connect gate="G" pin="/RAS" pad="U5"/>
<connect gate="G" pin="/RD" pad="U4"/>
<connect gate="G" pin="/SCAN_MODE" pad="K15"/>
<connect gate="G" pin="/WAIT" pad="T8"/>
<connect gate="G" pin="/WR" pad="V3"/>
<connect gate="G" pin="AI0+" pad="D13"/>
<connect gate="G" pin="AI0-" pad="A13"/>
<connect gate="G" pin="AI1+" pad="D14"/>
<connect gate="G" pin="AI1-" pad="A14"/>
<connect gate="G" pin="ALE" pad="T10"/>
<connect gate="G" pin="AO0+" pad="A15"/>
<connect gate="G" pin="AO0-" pad="B15"/>
<connect gate="G" pin="AO1+" pad="C14"/>
<connect gate="G" pin="AO1-" pad="B14"/>
<connect gate="G" pin="BFCLK0" pad="M2"/>
<connect gate="G" pin="BYPASS" pad="B17"/>
<connect gate="G" pin="CEXT" pad="A17"/>
<connect gate="G" pin="CKE" pad="U10"/>
<connect gate="G" pin="CLKOUT" pad="C17"/>
<connect gate="G" pin="CODEC_DIS" pad="C16"/>
<connect gate="G" pin="CS0" pad="R9"/>
<connect gate="G" pin="CS1" pad="R8"/>
<connect gate="G" pin="CS2" pad="R7"/>
<connect gate="G" pin="CS3" pad="V7"/>
<connect gate="G" pin="CS4" pad="V6"/>
<connect gate="G" pin="CS5" pad="V5"/>
<connect gate="G" pin="CS6" pad="U7"/>
<connect gate="G" pin="CSEMU" pad="V8"/>
<connect gate="G" pin="CSOVL" pad="T9"/>
<connect gate="G" pin="EBUCLK" pad="M1"/>
<connect gate="G" pin="HRST" pad="D16"/>
<connect gate="G" pin="MR/W" pad="V10"/>
<connect gate="G" pin="NMI" pad="A18"/>
<connect gate="G" pin="P4.0/AIN0" pad="C11"/>
<connect gate="G" pin="P4.1/AIN1" pad="A11"/>
<connect gate="G" pin="P4.2/AIN2" pad="B10"/>
<connect gate="G" pin="P4.3/AIN3" pad="A10"/>
<connect gate="G" pin="P4.4/AIN4" pad="C10"/>
<connect gate="G" pin="P4.5/AIN5" pad="A9"/>
<connect gate="G" pin="PLLCTRL_A0" pad="B8"/>
<connect gate="G" pin="PORST" pad="B18"/>
<connect gate="G" pin="TM_CTRL0" pad="B4"/>
<connect gate="G" pin="TM_CTRL1" pad="A3"/>
<connect gate="G" pin="VDDP_OSC" pad="D7"/>
<connect gate="G" pin="VDD_OSC1" pad="A7"/>
<connect gate="G" pin="VDD_OSC2" pad="C6"/>
<connect gate="G" pin="VSS_OSC" pad="B6"/>
<connect gate="G" pin="XTAL1" pad="A6"/>
<connect gate="G" pin="XTAL2" pad="B7"/>
<connect gate="G" pin="XTAL3" pad="A4"/>
<connect gate="G" pin="XTAL4" pad="B5"/>
<connect gate="P0" pin="0" pad="R18"/>
<connect gate="P0" pin="1" pad="N16"/>
<connect gate="P0" pin="2" pad="N17"/>
<connect gate="P0" pin="3" pad="P15"/>
<connect gate="P0" pin="4" pad="P18"/>
<connect gate="P0" pin="5" pad="N18"/>
<connect gate="P0" pin="6" pad="N15"/>
<connect gate="P0" pin="7" pad="M15"/>
<connect gate="P1" pin="0" pad="V18"/>
<connect gate="P1" pin="1" pad="R16"/>
<connect gate="P1" pin="2" pad="P16"/>
<connect gate="P1" pin="3" pad="T17"/>
<connect gate="P1" pin="4" pad="U18"/>
<connect gate="P1" pin="5" pad="R17"/>
<connect gate="P1" pin="6" pad="T18"/>
<connect gate="P1" pin="7" pad="P17"/>
<connect gate="P2" pin="0" pad="G18"/>
<connect gate="P2" pin="1" pad="G17"/>
<connect gate="P2" pin="10" pad="D18"/>
<connect gate="P2" pin="11" pad="C18"/>
<connect gate="P2" pin="12" pad="F16"/>
<connect gate="P2" pin="13" pad="D17"/>
<connect gate="P2" pin="14" pad="E16"/>
<connect gate="P2" pin="15" pad="F15"/>
<connect gate="P2" pin="2" pad="H16"/>
<connect gate="P2" pin="3" pad="F18"/>
<connect gate="P2" pin="4" pad="E18"/>
<connect gate="P2" pin="5" pad="F17"/>
<connect gate="P2" pin="6" pad="H15"/>
<connect gate="P2" pin="7" pad="G16"/>
<connect gate="P2" pin="8" pad="E17"/>
<connect gate="P2" pin="9" pad="G15"/>
<connect gate="P3" pin="0" pad="L15"/>
<connect gate="P3" pin="1" pad="M16"/>
<connect gate="P3" pin="10" pad="K16"/>
<connect gate="P3" pin="11" pad="J17"/>
<connect gate="P3" pin="12" pad="J15"/>
<connect gate="P3" pin="13" pad="H18"/>
<connect gate="P3" pin="14" pad="H17"/>
<connect gate="P3" pin="15" pad="J16"/>
<connect gate="P3" pin="2" pad="M17"/>
<connect gate="P3" pin="3" pad="M18"/>
<connect gate="P3" pin="4" pad="L17"/>
<connect gate="P3" pin="5" pad="L16"/>
<connect gate="P3" pin="6" pad="L18"/>
<connect gate="P3" pin="7" pad="K17"/>
<connect gate="P3" pin="8" pad="K18"/>
<connect gate="P3" pin="9" pad="J18"/>
<connect gate="P5/TRACE" pin="0" pad="V15"/>
<connect gate="P5/TRACE" pin="1" pad="U14"/>
<connect gate="P5/TRACE" pin="10" pad="V13"/>
<connect gate="P5/TRACE" pin="11" pad="U12"/>
<connect gate="P5/TRACE" pin="12" pad="T11"/>
<connect gate="P5/TRACE" pin="13" pad="V12"/>
<connect gate="P5/TRACE" pin="14" pad="U11"/>
<connect gate="P5/TRACE" pin="15" pad="V11"/>
<connect gate="P5/TRACE" pin="2" pad="T13"/>
<connect gate="P5/TRACE" pin="3" pad="R14"/>
<connect gate="P5/TRACE" pin="4" pad="V14"/>
<connect gate="P5/TRACE" pin="5" pad="R13"/>
<connect gate="P5/TRACE" pin="6" pad="U13"/>
<connect gate="P5/TRACE" pin="7" pad="T12"/>
<connect gate="P5/TRACE" pin="8" pad="R12"/>
<connect gate="P5/TRACE" pin="9" pad="R11"/>
<connect gate="PWR" pin="1V8@0" pad="A16"/>
<connect gate="PWR" pin="1V8@1" pad="B16"/>
<connect gate="PWR" pin="1V8@2" pad="B3"/>
<connect gate="PWR" pin="1V8@3" pad="C4"/>
<connect gate="PWR" pin="1V8@4" pad="D5"/>
<connect gate="PWR" pin="1V8@5" pad="J4"/>
<connect gate="PWR" pin="1V8@6" pad="L4"/>
<connect gate="PWR" pin="1V8@7" pad="R4"/>
<connect gate="PWR" pin="3V3@0" pad="G11"/>
<connect gate="PWR" pin="3V3@1" pad="G12"/>
<connect gate="PWR" pin="3V3@10" pad="M7"/>
<connect gate="PWR" pin="3V3@11" pad="M8"/>
<connect gate="PWR" pin="3V3@2" pad="G7"/>
<connect gate="PWR" pin="3V3@3" pad="G8"/>
<connect gate="PWR" pin="3V3@4" pad="H12"/>
<connect gate="PWR" pin="3V3@5" pad="H7"/>
<connect gate="PWR" pin="3V3@6" pad="L12"/>
<connect gate="PWR" pin="3V3@7" pad="L7"/>
<connect gate="PWR" pin="3V3@8" pad="M11"/>
<connect gate="PWR" pin="3V3@9" pad="M12"/>
<connect gate="PWR" pin="GND@0" pad="A1"/>
<connect gate="PWR" pin="GND@1" pad="B2"/>
<connect gate="PWR" pin="GND@10" pad="H9"/>
<connect gate="PWR" pin="GND@11" pad="J10"/>
<connect gate="PWR" pin="GND@12" pad="J11"/>
<connect gate="PWR" pin="GND@13" pad="J12"/>
<connect gate="PWR" pin="GND@14" pad="J7"/>
<connect gate="PWR" pin="GND@15" pad="J8"/>
<connect gate="PWR" pin="GND@16" pad="J9"/>
<connect gate="PWR" pin="GND@17" pad="K10"/>
<connect gate="PWR" pin="GND@18" pad="K11"/>
<connect gate="PWR" pin="GND@19" pad="K12"/>
<connect gate="PWR" pin="GND@2" pad="C3"/>
<connect gate="PWR" pin="GND@20" pad="K7"/>
<connect gate="PWR" pin="GND@21" pad="K8"/>
<connect gate="PWR" pin="GND@22" pad="K9"/>
<connect gate="PWR" pin="GND@23" pad="L10"/>
<connect gate="PWR" pin="GND@24" pad="L11"/>
<connect gate="PWR" pin="GND@25" pad="L8"/>
<connect gate="PWR" pin="GND@26" pad="L9"/>
<connect gate="PWR" pin="GND@27" pad="M10"/>
<connect gate="PWR" pin="GND@28" pad="M9"/>
<connect gate="PWR" pin="GND@3" pad="D4"/>
<connect gate="PWR" pin="GND@4" pad="D6"/>
<connect gate="PWR" pin="GND@5" pad="G10"/>
<connect gate="PWR" pin="GND@6" pad="G9"/>
<connect gate="PWR" pin="GND@7" pad="H10"/>
<connect gate="PWR" pin="GND@8" pad="H11"/>
<connect gate="PWR" pin="GND@9" pad="H8"/>
<connect gate="PWR2" pin="VAGND_ADC" pad="B11"/>
<connect gate="PWR2" pin="VAREF_ADC" pad="D11"/>
<connect gate="PWR2" pin="VDDP_ADC" pad="C12"/>
<connect gate="PWR2" pin="VDDP_COD@0" pad="E15"/>
<connect gate="PWR2" pin="VDDP_OSC@1" pad="C7"/>
<connect gate="PWR2" pin="VDDR@0" pad="A2"/>
<connect gate="PWR2" pin="VDDR@1" pad="C5"/>
<connect gate="PWR2" pin="VDD_GUARD" pad="C9"/>
<connect gate="PWR2" pin="VDD_PLL" pad="D9"/>
<connect gate="PWR2" pin="VDD_SB" pad="R15"/>
<connect gate="PWR2" pin="VGND_COD" pad="C13"/>
<connect gate="PWR2" pin="VREF_COD" pad="B13"/>
<connect gate="PWR2" pin="VSSA_ADC" pad="A12"/>
<connect gate="PWR2" pin="VSSA_COD@0" pad="D15"/>
<connect gate="PWR2" pin="VSSP_ADC@0" pad="B12"/>
<connect gate="PWR2" pin="VSSP_ADC@1" pad="D12"/>
<connect gate="PWR2" pin="VSSP_ADC@2" pad="D10"/>
<connect gate="PWR2" pin="VSSP_COD@0" pad="C15"/>
<connect gate="PWR2" pin="VSSP_OSC@0" pad="D8"/>
<connect gate="PWR2" pin="VSSP_OSC@1" pad="A5"/>
<connect gate="PWR2" pin="VSS_GUARD@1" pad="A8"/>
<connect gate="PWR2" pin="VSS_GUARD@2" pad="C8"/>
<connect gate="PWR2" pin="VSS_PLL" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC11IB" prefix="IC">
<description>&lt;b&gt;32-Bit Single-Chip Microcontroller TriCore Family&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. TC11IB_DS_v24.pdf</description>
<gates>
<gate name="-C" symbol="TC11IB"/>
<gate name="-PCI" symbol="PCI"/>
<gate name="-AD" symbol="AD31"/>
<gate name="-JTAG" symbol="ODCS/JTAG"/>
<gate name="-P0" symbol="PORT16"/>
<gate name="-P1" symbol="PORT16"/>
<gate name="-P2" symbol="PORT16"/>
<gate name="-P3" symbol="PORT16"/>
<gate name="-P4" symbol="PORT16"/>
<gate name="-P5" symbol="PORT16"/>
<gate name="-P_AD" symbol="AD31"/>
<gate name="-A" symbol="A23"/>
<gate name="-VSS1" symbol="VSS"/>
<gate name="-VSS2" symbol="VSS"/>
<gate name="-VSS3" symbol="VSS"/>
<gate name="-VSS4" symbol="VSS"/>
<gate name="-VSS5" symbol="VSS"/>
<gate name="-VSS6" symbol="VSS"/>
<gate name="-VSS7" symbol="VSS"/>
<gate name="-VSS8" symbol="VSS"/>
<gate name="-VSS9" symbol="VSS"/>
<gate name="-VSS10" symbol="VSS"/>
<gate name="-VSS11" symbol="VSS"/>
<gate name="-VSS12" symbol="VSS"/>
<gate name="-VSS13" symbol="VSS"/>
<gate name="-VSS14" symbol="VSS"/>
<gate name="-VSS15" symbol="VSS"/>
<gate name="-VSS16" symbol="VSS"/>
<gate name="-VSS17" symbol="VSS"/>
<gate name="-VSS18" symbol="VSS"/>
<gate name="-VSS19" symbol="VSS"/>
<gate name="-VSS20" symbol="VSS"/>
<gate name="-VSS21" symbol="VSS"/>
<gate name="-VSS22" symbol="VSS"/>
<gate name="-VSS23" symbol="VSS"/>
<gate name="-VSS24" symbol="VSS"/>
<gate name="-VSS25" symbol="VSS"/>
<gate name="-VSS26" symbol="VSS"/>
<gate name="-VSS27" symbol="VSS"/>
<gate name="-VSS28" symbol="VSS"/>
<gate name="-VSS29" symbol="VSS"/>
<gate name="-VSS30" symbol="VSS"/>
<gate name="-VSS31" symbol="VSS"/>
<gate name="-VSS32" symbol="VSS"/>
<gate name="-VSS33" symbol="VSS"/>
<gate name="-VSS34" symbol="VSS"/>
<gate name="-VSS35" symbol="VSS"/>
<gate name="-VSS36" symbol="VSS"/>
<gate name="-VSS37" symbol="VSS"/>
<gate name="-VSS38" symbol="VSS"/>
<gate name="-VSS39" symbol="VSS"/>
<gate name="-VSS40" symbol="VSS"/>
<gate name="-VSS41" symbol="VSS"/>
<gate name="-VSS42" symbol="VSS"/>
<gate name="-VSS43" symbol="VSS"/>
<gate name="-VSS44" symbol="VSS"/>
<gate name="-VSS45" symbol="VSS"/>
<gate name="-VSS46" symbol="VSS"/>
<gate name="-VSS47" symbol="VSS"/>
<gate name="-VSS48" symbol="VSS"/>
<gate name="-VSS49" symbol="VSS"/>
<gate name="-VSS50" symbol="VSS"/>
<gate name="-VSS51" symbol="VSS"/>
<gate name="-VSS52" symbol="VSS"/>
<gate name="VDDP1" symbol="VDDP"/>
<gate name="VDDP2" symbol="VDDP"/>
<gate name="VDDP3" symbol="VDDP"/>
<gate name="VDDP4" symbol="VDDP"/>
<gate name="VDDP5" symbol="VDDP"/>
<gate name="VDDP6" symbol="VDDP"/>
<gate name="VDDP7" symbol="VDDP"/>
<gate name="VDDP8" symbol="VDDP"/>
<gate name="VDDP9" symbol="VDDP"/>
<gate name="VDDP10" symbol="VDDP"/>
<gate name="VDDP11" symbol="VDDP"/>
<gate name="VDDP12" symbol="VDDP"/>
<gate name="VDDP13" symbol="VDDP"/>
<gate name="VDDP14" symbol="VDDP"/>
<gate name="VDDP15" symbol="VDDP"/>
<gate name="VDDP16" symbol="VDDP"/>
<gate name="VDDP17" symbol="VDDP"/>
<gate name="VDDP18" symbol="VDDP"/>
<gate name="VDDP19" symbol="VDDP"/>
<gate name="VDDP20" symbol="VDDP"/>
<gate name="VDD1" symbol="VDD"/>
<gate name="VDD2" symbol="VDD"/>
<gate name="VDD3" symbol="VDD"/>
<gate name="VDD4" symbol="VDD"/>
<gate name="VDD5" symbol="VDD"/>
<gate name="VDD6" symbol="VDD"/>
<gate name="VDD7" symbol="VDD"/>
<gate name="VDD8" symbol="VDD"/>
<gate name="VDD9" symbol="VDD"/>
<gate name="VDD10" symbol="VDD"/>
<gate name="VDD11" symbol="VDD"/>
<gate name="VDD12" symbol="VDD"/>
<gate name="VDD13" symbol="VDD"/>
<gate name="VDD14" symbol="VDD"/>
<gate name="VDD15" symbol="VDD"/>
<gate name="VDD16" symbol="VDD"/>
<gate name="VDD17" symbol="VDD"/>
<gate name="VDD18" symbol="VDD"/>
<gate name="VDD19" symbol="VDD"/>
<gate name="VDD20" symbol="VDD"/>
<gate name="VDD21" symbol="VDD"/>
</gates>
<devices>
<device name="" package="P-BGA-388-2">
<connects>
<connect gate="-A" pin="A0" pad="AA26"/>
<connect gate="-A" pin="A1" pad="V24"/>
<connect gate="-A" pin="A10" pad="V26"/>
<connect gate="-A" pin="A11" pad="U25"/>
<connect gate="-A" pin="A12" pad="U24"/>
<connect gate="-A" pin="A13" pad="U26"/>
<connect gate="-A" pin="A14" pad="T26"/>
<connect gate="-A" pin="A15" pad="T25"/>
<connect gate="-A" pin="A16" pad="T24"/>
<connect gate="-A" pin="A17" pad="R23"/>
<connect gate="-A" pin="A18" pad="R24"/>
<connect gate="-A" pin="A19" pad="R25"/>
<connect gate="-A" pin="A2" pad="W24"/>
<connect gate="-A" pin="A20" pad="A24"/>
<connect gate="-A" pin="A21" pad="B23"/>
<connect gate="-A" pin="A22" pad="C23"/>
<connect gate="-A" pin="A23" pad="D22"/>
<connect gate="-A" pin="A3" pad="Y24"/>
<connect gate="-A" pin="A4" pad="Y25"/>
<connect gate="-A" pin="A5" pad="AA25"/>
<connect gate="-A" pin="A6" pad="Y26"/>
<connect gate="-A" pin="A7" pad="W25"/>
<connect gate="-A" pin="A8" pad="W26"/>
<connect gate="-A" pin="A9" pad="V25"/>
<connect gate="-AD" pin="AD0" pad="L25"/>
<connect gate="-AD" pin="AD1" pad="L24"/>
<connect gate="-AD" pin="AD10" pad="J25"/>
<connect gate="-AD" pin="AD11" pad="H26"/>
<connect gate="-AD" pin="AD12" pad="H25"/>
<connect gate="-AD" pin="AD13" pad="G26"/>
<connect gate="-AD" pin="AD14" pad="G25"/>
<connect gate="-AD" pin="AD15" pad="F26"/>
<connect gate="-AD" pin="AD16" pad="F25"/>
<connect gate="-AD" pin="AD17" pad="F24"/>
<connect gate="-AD" pin="AD18" pad="E24"/>
<connect gate="-AD" pin="AD19" pad="E23"/>
<connect gate="-AD" pin="AD2" pad="K24"/>
<connect gate="-AD" pin="AD20" pad="D24"/>
<connect gate="-AD" pin="AD21" pad="C25"/>
<connect gate="-AD" pin="AD22" pad="C24"/>
<connect gate="-AD" pin="AD23" pad="B24"/>
<connect gate="-AD" pin="AD24" pad="E26"/>
<connect gate="-AD" pin="AD25" pad="E25"/>
<connect gate="-AD" pin="AD26" pad="D26"/>
<connect gate="-AD" pin="AD27" pad="D25"/>
<connect gate="-AD" pin="AD28" pad="C26"/>
<connect gate="-AD" pin="AD29" pad="B26"/>
<connect gate="-AD" pin="AD3" pad="K25"/>
<connect gate="-AD" pin="AD30" pad="B25"/>
<connect gate="-AD" pin="AD31" pad="A25"/>
<connect gate="-AD" pin="AD4" pad="J24"/>
<connect gate="-AD" pin="AD5" pad="H24"/>
<connect gate="-AD" pin="AD6" pad="G24"/>
<connect gate="-AD" pin="AD7" pad="G23"/>
<connect gate="-AD" pin="AD8" pad="K26"/>
<connect gate="-AD" pin="AD9" pad="J26"/>
<connect gate="-C" pin="!ADV" pad="B19"/>
<connect gate="-C" pin="!BAA" pad="A22"/>
<connect gate="-C" pin="!BC0" pad="M25"/>
<connect gate="-C" pin="!BC1" pad="M26"/>
<connect gate="-C" pin="!BC2" pad="L26"/>
<connect gate="-C" pin="!BC3" pad="M24"/>
<connect gate="-C" pin="!BREQ" pad="B22"/>
<connect gate="-C" pin="!BRKIN" pad="H3"/>
<connect gate="-C" pin="!BRKOUT" pad="J3"/>
<connect gate="-C" pin="!CAS" pad="N25"/>
<connect gate="-C" pin="!CKE" pad="P26"/>
<connect gate="-C" pin="!CMDELAY" pad="B21"/>
<connect gate="-C" pin="!CS0" pad="AB24"/>
<connect gate="-C" pin="!CS1" pad="AC26"/>
<connect gate="-C" pin="!CS2" pad="AB25"/>
<connect gate="-C" pin="!CS3" pad="AA24"/>
<connect gate="-C" pin="!CS4" pad="Y23"/>
<connect gate="-C" pin="!CS5" pad="R26"/>
<connect gate="-C" pin="!CS6" pad="P24"/>
<connect gate="-C" pin="!CSEMU" pad="AC25"/>
<connect gate="-C" pin="!CSFPI" pad="B20"/>
<connect gate="-C" pin="!CSGLB" pad="A21"/>
<connect gate="-C" pin="!CSOVL" pad="C20"/>
<connect gate="-C" pin="!HDRST" pad="A1"/>
<connect gate="-C" pin="!HLDA" pad="A23"/>
<connect gate="-C" pin="!HOLD" pad="C22"/>
<connect gate="-C" pin="!MR_W" pad="C21"/>
<connect gate="-C" pin="!NMI" pad="B2"/>
<connect gate="-C" pin="!OCDSE" pad="H2"/>
<connect gate="-C" pin="!PORST" pad="C3"/>
<connect gate="-C" pin="!RAS" pad="P25"/>
<connect gate="-C" pin="!RD" pad="AB26"/>
<connect gate="-C" pin="!RDWR" pad="N24"/>
<connect gate="-C" pin="!RMW" pad="AB23"/>
<connect gate="-C" pin="!SVM" pad="D20"/>
<connect gate="-C" pin="!TM_CTRL1" pad="C15"/>
<connect gate="-C" pin="!TM_CTRL2" pad="C12"/>
<connect gate="-C" pin="!WAIT" pad="C19"/>
<connect gate="-C" pin="ACLK" pad="M23"/>
<connect gate="-C" pin="ALE" pad="A20"/>
<connect gate="-C" pin="CFG0" pad="K2"/>
<connect gate="-C" pin="CFG1" pad="K3"/>
<connect gate="-C" pin="CFG2" pad="J1"/>
<connect gate="-C" pin="CFG3" pad="J2"/>
<connect gate="-C" pin="CLK42" pad="D12"/>
<connect gate="-C" pin="CPUCLK" pad="C2"/>
<connect gate="-C" pin="EBUCLK" pad="N26"/>
<connect gate="-C" pin="MII_MDIO" pad="A10"/>
<connect gate="-C" pin="MII_RXCLK" pad="C11"/>
<connect gate="-C" pin="MII_TXCLK" pad="A11"/>
<connect gate="-C" pin="PLL42_CTRL" pad="B12"/>
<connect gate="-C" pin="PLL96_CTRL" pad="B15"/>
<connect gate="-C" pin="RESERVED@1" pad="A26"/>
<connect gate="-C" pin="RESERVED@2" pad="D15"/>
<connect gate="-C" pin="RESERVED@3" pad="AE26"/>
<connect gate="-C" pin="RESERVED@4" pad="AF9"/>
<connect gate="-C" pin="RESERVED@5" pad="AF26"/>
<connect gate="-C" pin="TESTMODE" pad="AE9"/>
<connect gate="-C" pin="VCOMREF" pad="AD10"/>
<connect gate="-C" pin="VDDDRAM@1" pad="A17"/>
<connect gate="-C" pin="VDDDRAM@2" pad="AF13"/>
<connect gate="-C" pin="VDDOSC" pad="B14"/>
<connect gate="-C" pin="VDDPLL42" pad="A12"/>
<connect gate="-C" pin="VDDPLL96" pad="B13"/>
<connect gate="-C" pin="VLMUREF" pad="A16"/>
<connect gate="-C" pin="VSSOSC" pad="C14"/>
<connect gate="-C" pin="VSSPLL42" pad="C13"/>
<connect gate="-C" pin="VSSPLL96" pad="A13"/>
<connect gate="-C" pin="XTAL1" pad="A15"/>
<connect gate="-C" pin="XTAL2" pad="A14"/>
<connect gate="-JTAG" pin="!TRST" pad="AE8"/>
<connect gate="-JTAG" pin="OCDS2BRK0" pad="G2"/>
<connect gate="-JTAG" pin="OCDS2BRK1" pad="G3"/>
<connect gate="-JTAG" pin="OCDS2BRK2" pad="G4"/>
<connect gate="-JTAG" pin="OCDS2PC0" pad="G1"/>
<connect gate="-JTAG" pin="OCDS2PC1" pad="F1"/>
<connect gate="-JTAG" pin="OCDS2PC2" pad="F2"/>
<connect gate="-JTAG" pin="OCDS2PC3" pad="E1"/>
<connect gate="-JTAG" pin="OCDS2PC4" pad="D1"/>
<connect gate="-JTAG" pin="OCDS2PC5" pad="F3"/>
<connect gate="-JTAG" pin="OCDS2PC6" pad="E2"/>
<connect gate="-JTAG" pin="OCDS2PC7" pad="C1"/>
<connect gate="-JTAG" pin="OCDS2PS0" pad="E3"/>
<connect gate="-JTAG" pin="OCDS2PS1" pad="D2"/>
<connect gate="-JTAG" pin="OCDS2PS2" pad="B1"/>
<connect gate="-JTAG" pin="OCDS2PS3" pad="E4"/>
<connect gate="-JTAG" pin="OCDS2PS4" pad="D3"/>
<connect gate="-JTAG" pin="TCK" pad="AF7"/>
<connect gate="-JTAG" pin="TDI" pad="AD9"/>
<connect gate="-JTAG" pin="TDO" pad="AF8"/>
<connect gate="-JTAG" pin="TMS" pad="AD8"/>
<connect gate="-P0" pin="0" pad="K1"/>
<connect gate="-P0" pin="1" pad="L3"/>
<connect gate="-P0" pin="10" pad="N3"/>
<connect gate="-P0" pin="11" pad="P1"/>
<connect gate="-P0" pin="12" pad="P2"/>
<connect gate="-P0" pin="13" pad="P3"/>
<connect gate="-P0" pin="14" pad="R1"/>
<connect gate="-P0" pin="15" pad="R2"/>
<connect gate="-P0" pin="2" pad="L2"/>
<connect gate="-P0" pin="3" pad="L1"/>
<connect gate="-P0" pin="4" pad="M1"/>
<connect gate="-P0" pin="5" pad="M2"/>
<connect gate="-P0" pin="6" pad="M3"/>
<connect gate="-P0" pin="7" pad="M4"/>
<connect gate="-P0" pin="8" pad="N1"/>
<connect gate="-P0" pin="9" pad="N2"/>
<connect gate="-P1" pin="0" pad="A7"/>
<connect gate="-P1" pin="1" pad="B7"/>
<connect gate="-P1" pin="10" pad="D5"/>
<connect gate="-P1" pin="11" pad="A4"/>
<connect gate="-P1" pin="12" pad="C4"/>
<connect gate="-P1" pin="13" pad="A3"/>
<connect gate="-P1" pin="14" pad="B3"/>
<connect gate="-P1" pin="15" pad="A2"/>
<connect gate="-P1" pin="2" pad="C7"/>
<connect gate="-P1" pin="3" pad="D7"/>
<connect gate="-P1" pin="4" pad="A6"/>
<connect gate="-P1" pin="5" pad="B6"/>
<connect gate="-P1" pin="6" pad="C6"/>
<connect gate="-P1" pin="7" pad="A5"/>
<connect gate="-P1" pin="8" pad="B5"/>
<connect gate="-P1" pin="9" pad="C5"/>
<connect gate="-P2" pin="0" pad="C18"/>
<connect gate="-P2" pin="1" pad="A19"/>
<connect gate="-P2" pin="10" pad="A9"/>
<connect gate="-P2" pin="11" pad="B9"/>
<connect gate="-P2" pin="12" pad="A8"/>
<connect gate="-P2" pin="13" pad="C9"/>
<connect gate="-P2" pin="14" pad="B8"/>
<connect gate="-P2" pin="15" pad="C8"/>
<connect gate="-P2" pin="2" pad="B18"/>
<connect gate="-P2" pin="3" pad="A18"/>
<connect gate="-P2" pin="4" pad="C17"/>
<connect gate="-P2" pin="5" pad="B17"/>
<connect gate="-P2" pin="6" pad="C16"/>
<connect gate="-P2" pin="7" pad="B16"/>
<connect gate="-P2" pin="8" pad="B10"/>
<connect gate="-P2" pin="9" pad="C10"/>
<connect gate="-P3" pin="0" pad="R3"/>
<connect gate="-P3" pin="1" pad="R4"/>
<connect gate="-P3" pin="10" pad="W2"/>
<connect gate="-P3" pin="11" pad="W3"/>
<connect gate="-P3" pin="12" pad="Y1"/>
<connect gate="-P3" pin="13" pad="Y2"/>
<connect gate="-P3" pin="14" pad="Y3"/>
<connect gate="-P3" pin="15" pad="X4"/>
<connect gate="-P3" pin="2" pad="T1"/>
<connect gate="-P3" pin="3" pad="T3"/>
<connect gate="-P3" pin="4" pad="U1"/>
<connect gate="-P3" pin="5" pad="U2"/>
<connect gate="-P3" pin="6" pad="U3"/>
<connect gate="-P3" pin="7" pad="V1"/>
<connect gate="-P3" pin="8" pad="V2"/>
<connect gate="-P3" pin="9" pad="V3"/>
<connect gate="-P4" pin="0" pad="AA1"/>
<connect gate="-P4" pin="1" pad="AA2"/>
<connect gate="-P4" pin="10" pad="AD1"/>
<connect gate="-P4" pin="11" pad="AD2"/>
<connect gate="-P4" pin="12" pad="AE1"/>
<connect gate="-P4" pin="13" pad="AE2"/>
<connect gate="-P4" pin="14" pad="AD3"/>
<connect gate="-P4" pin="15" pad="AF2"/>
<connect gate="-P4" pin="2" pad="AA3"/>
<connect gate="-P4" pin="3" pad="AB1"/>
<connect gate="-P4" pin="4" pad="AB2"/>
<connect gate="-P4" pin="5" pad="AB3"/>
<connect gate="-P4" pin="6" pad="AB4"/>
<connect gate="-P4" pin="7" pad="AC1"/>
<connect gate="-P4" pin="8" pad="AC2"/>
<connect gate="-P4" pin="9" pad="AC3"/>
<connect gate="-P5" pin="0" pad="AF1"/>
<connect gate="-P5" pin="1" pad="AE3"/>
<connect gate="-P5" pin="10" pad="AC7"/>
<connect gate="-P5" pin="11" pad="AF5"/>
<connect gate="-P5" pin="12" pad="AE6"/>
<connect gate="-P5" pin="13" pad="AD7"/>
<connect gate="-P5" pin="14" pad="AF6"/>
<connect gate="-P5" pin="15" pad="AE7"/>
<connect gate="-P5" pin="2" pad="AD4"/>
<connect gate="-P5" pin="3" pad="AC5"/>
<connect gate="-P5" pin="4" pad="AF3"/>
<connect gate="-P5" pin="5" pad="AE4"/>
<connect gate="-P5" pin="6" pad="AD5"/>
<connect gate="-P5" pin="7" pad="AF4"/>
<connect gate="-P5" pin="8" pad="AE5"/>
<connect gate="-P5" pin="9" pad="AD6"/>
<connect gate="-PCI" pin="!P_CBE0" pad="AC24"/>
<connect gate="-PCI" pin="!P_CBE1" pad="AF21"/>
<connect gate="-PCI" pin="!P_CBE2" pad="AF18"/>
<connect gate="-PCI" pin="!P_CBE3" pad="AF15"/>
<connect gate="-PCI" pin="!P_DEVSEL" pad="AF19"/>
<connect gate="-PCI" pin="!P_FRAME" pad="AD18"/>
<connect gate="-PCI" pin="!P_GNT" pad="AD11"/>
<connect gate="-PCI" pin="!P_INTA" pad="AE10"/>
<connect gate="-PCI" pin="!P_INTB" pad="AF10"/>
<connect gate="-PCI" pin="!P_IRDY" pad="AE18"/>
<connect gate="-PCI" pin="!P_LOCK" pad="AE19"/>
<connect gate="-PCI" pin="!P_PERR" pad="AF20"/>
<connect gate="-PCI" pin="!P_PME" pad="AC12"/>
<connect gate="-PCI" pin="!P_REQ" pad="AE11"/>
<connect gate="-PCI" pin="!P_SERR" pad="AE20"/>
<connect gate="-PCI" pin="!P_STOP" pad="AC20"/>
<connect gate="-PCI" pin="!P_TRDY" pad="AD19"/>
<connect gate="-PCI" pin="P_CLK33" pad="AF11"/>
<connect gate="-PCI" pin="P_IDSEL" pad="AC15"/>
<connect gate="-PCI" pin="P_PAR" pad="AD20"/>
<connect gate="-P_AD" pin="AD0" pad="AD26"/>
<connect gate="-P_AD" pin="AD1" pad="AE25"/>
<connect gate="-P_AD" pin="AD10" pad="AE22"/>
<connect gate="-P_AD" pin="AD11" pad="AD22"/>
<connect gate="-P_AD" pin="AD12" pad="AF22"/>
<connect gate="-P_AD" pin="AD13" pad="AC22"/>
<connect gate="-P_AD" pin="AD14" pad="AE21"/>
<connect gate="-P_AD" pin="AD15" pad="AD21"/>
<connect gate="-P_AD" pin="AD16" pad="AE17"/>
<connect gate="-P_AD" pin="AD17" pad="AF17"/>
<connect gate="-P_AD" pin="AD18" pad="AD17"/>
<connect gate="-P_AD" pin="AD19" pad="AE16"/>
<connect gate="-P_AD" pin="AD2" pad="AD25"/>
<connect gate="-P_AD" pin="AD20" pad="AD16"/>
<connect gate="-P_AD" pin="AD21" pad="AF16"/>
<connect gate="-P_AD" pin="AD22" pad="AD15"/>
<connect gate="-P_AD" pin="AD23" pad="AE15"/>
<connect gate="-P_AD" pin="AD24" pad="AE14"/>
<connect gate="-P_AD" pin="AD25" pad="AF14"/>
<connect gate="-P_AD" pin="AD26" pad="AD14"/>
<connect gate="-P_AD" pin="AD27" pad="AE13"/>
<connect gate="-P_AD" pin="AD28" pad="AD13"/>
<connect gate="-P_AD" pin="AD29" pad="AE12"/>
<connect gate="-P_AD" pin="AD3" pad="AF25"/>
<connect gate="-P_AD" pin="AD30" pad="AD12"/>
<connect gate="-P_AD" pin="AD31" pad="AF12"/>
<connect gate="-P_AD" pin="AD4" pad="AE24"/>
<connect gate="-P_AD" pin="AD5" pad="AF24"/>
<connect gate="-P_AD" pin="AD6" pad="AD24"/>
<connect gate="-P_AD" pin="AD7" pad="AE23"/>
<connect gate="-P_AD" pin="AD8" pad="AF23"/>
<connect gate="-P_AD" pin="AD9" pad="AD23"/>
<connect gate="-VSS1" pin="VSS" pad="D4"/>
<connect gate="-VSS10" pin="VSS" pad="V4"/>
<connect gate="-VSS11" pin="VSS" pad="V23"/>
<connect gate="-VSS12" pin="VSS" pad="AC4"/>
<connect gate="-VSS13" pin="VSS" pad="AC9"/>
<connect gate="-VSS14" pin="VSS" pad="AC14"/>
<connect gate="-VSS15" pin="VSS" pad="AC18"/>
<connect gate="-VSS16" pin="VSS" pad="AC23"/>
<connect gate="-VSS17" pin="VSS" pad="L11"/>
<connect gate="-VSS18" pin="VSS" pad="L12"/>
<connect gate="-VSS19" pin="VSS" pad="L13"/>
<connect gate="-VSS2" pin="VSS" pad="D9"/>
<connect gate="-VSS20" pin="VSS" pad="L14"/>
<connect gate="-VSS21" pin="VSS" pad="L15"/>
<connect gate="-VSS22" pin="VSS" pad="L16"/>
<connect gate="-VSS23" pin="VSS" pad="M11"/>
<connect gate="-VSS24" pin="VSS" pad="M12"/>
<connect gate="-VSS25" pin="VSS" pad="M13"/>
<connect gate="-VSS26" pin="VSS" pad="M14"/>
<connect gate="-VSS27" pin="VSS" pad="M15"/>
<connect gate="-VSS28" pin="VSS" pad="M16"/>
<connect gate="-VSS29" pin="VSS" pad="N11"/>
<connect gate="-VSS3" pin="VSS" pad="D13"/>
<connect gate="-VSS30" pin="VSS" pad="N12"/>
<connect gate="-VSS31" pin="VSS" pad="N13"/>
<connect gate="-VSS32" pin="VSS" pad="N14"/>
<connect gate="-VSS33" pin="VSS" pad="N15"/>
<connect gate="-VSS34" pin="VSS" pad="N16"/>
<connect gate="-VSS35" pin="VSS" pad="P11"/>
<connect gate="-VSS36" pin="VSS" pad="P12"/>
<connect gate="-VSS37" pin="VSS" pad="P13"/>
<connect gate="-VSS38" pin="VSS" pad="P14"/>
<connect gate="-VSS39" pin="VSS" pad="P15"/>
<connect gate="-VSS4" pin="VSS" pad="D18"/>
<connect gate="-VSS40" pin="VSS" pad="P16"/>
<connect gate="-VSS41" pin="VSS" pad="R11"/>
<connect gate="-VSS42" pin="VSS" pad="R12"/>
<connect gate="-VSS43" pin="VSS" pad="R13"/>
<connect gate="-VSS44" pin="VSS" pad="R14"/>
<connect gate="-VSS45" pin="VSS" pad="R15"/>
<connect gate="-VSS46" pin="VSS" pad="R16"/>
<connect gate="-VSS47" pin="VSS" pad="T11"/>
<connect gate="-VSS48" pin="VSS" pad="T12"/>
<connect gate="-VSS49" pin="VSS" pad="T13"/>
<connect gate="-VSS5" pin="VSS" pad="D23"/>
<connect gate="-VSS50" pin="VSS" pad="T14"/>
<connect gate="-VSS51" pin="VSS" pad="T15"/>
<connect gate="-VSS52" pin="VSS" pad="T16"/>
<connect gate="-VSS6" pin="VSS" pad="J4"/>
<connect gate="-VSS7" pin="VSS" pad="J23"/>
<connect gate="-VSS8" pin="VSS" pad="N23"/>
<connect gate="-VSS9" pin="VSS" pad="P4"/>
<connect gate="VDD1" pin="VDD" pad="H1"/>
<connect gate="VDD10" pin="VDD" pad="D21"/>
<connect gate="VDD11" pin="VDD" pad="F23"/>
<connect gate="VDD12" pin="VDD" pad="K4"/>
<connect gate="VDD13" pin="VDD" pad="K23"/>
<connect gate="VDD14" pin="VDD" pad="U4"/>
<connect gate="VDD15" pin="VDD" pad="U23"/>
<connect gate="VDD16" pin="VDD" pad="AA4"/>
<connect gate="VDD17" pin="VDD" pad="AA23"/>
<connect gate="VDD18" pin="VDD" pad="AC6"/>
<connect gate="VDD19" pin="VDD" pad="AC10"/>
<connect gate="VDD2" pin="VDD" pad="W1"/>
<connect gate="VDD20" pin="VDD" pad="AC17"/>
<connect gate="VDD21" pin="VDD" pad="AC21"/>
<connect gate="VDD3" pin="VDD" pad="T2"/>
<connect gate="VDD4" pin="VDD" pad="B4"/>
<connect gate="VDD5" pin="VDD" pad="B11"/>
<connect gate="VDD6" pin="VDD" pad="D6"/>
<connect gate="VDD7" pin="VDD" pad="F4"/>
<connect gate="VDD8" pin="VDD" pad="D10"/>
<connect gate="VDD9" pin="VDD" pad="D17"/>
<connect gate="VDDP1" pin="VDDP" pad="D8"/>
<connect gate="VDDP10" pin="VDDP" pad="N4"/>
<connect gate="VDDP11" pin="VDDP" pad="P23"/>
<connect gate="VDDP12" pin="VDDP" pad="T4"/>
<connect gate="VDDP13" pin="VDDP" pad="T23"/>
<connect gate="VDDP14" pin="VDDP" pad="W4"/>
<connect gate="VDDP15" pin="VDDP" pad="W23"/>
<connect gate="VDDP16" pin="VDDP" pad="AC8"/>
<connect gate="VDDP17" pin="VDDP" pad="AC11"/>
<connect gate="VDDP18" pin="VDDP" pad="AC13"/>
<connect gate="VDDP19" pin="VDDP" pad="AC16"/>
<connect gate="VDDP2" pin="VDDP" pad="D11"/>
<connect gate="VDDP20" pin="VDDP" pad="AC19"/>
<connect gate="VDDP3" pin="VDDP" pad="D14"/>
<connect gate="VDDP4" pin="VDDP" pad="D16"/>
<connect gate="VDDP5" pin="VDDP" pad="D19"/>
<connect gate="VDDP6" pin="VDDP" pad="H4"/>
<connect gate="VDDP7" pin="VDDP" pad="H23"/>
<connect gate="VDDP8" pin="VDDP" pad="L4"/>
<connect gate="VDDP9" pin="VDDP" pad="L23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1130" prefix="IC">
<description>&lt;b&gt; 32-Bit Industrial &amp;Communication Controller&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. TC1130_DS_v031.pdf</description>
<gates>
<gate name="G" symbol="TC1130"/>
<gate name="PWR" symbol="PWR_TC1130"/>
<gate name="P0" symbol="PORT16"/>
<gate name="P1" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="P3" symbol="PORT16"/>
<gate name="RES" symbol="NC4"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="G" pin="/ADV" pad="B11"/>
<connect gate="G" pin="/BAA" pad="A11"/>
<connect gate="G" pin="/BRKIN" pad="T5"/>
<connect gate="G" pin="/CAS" pad="D5"/>
<connect gate="G" pin="/CSCOMB" pad="N3"/>
<connect gate="G" pin="/HDRST" pad="N5"/>
<connect gate="G" pin="/MR_W" pad="P3"/>
<connect gate="G" pin="/PORST" pad="R5"/>
<connect gate="G" pin="/RAS" pad="D6"/>
<connect gate="G" pin="/RD" pad="P2"/>
<connect gate="G" pin="/WAIT" pad="B9"/>
<connect gate="G" pin="/WR" pad="T3"/>
<connect gate="G" pin="A0" pad="K1"/>
<connect gate="G" pin="A1" pad="L1"/>
<connect gate="G" pin="A10" pad="J3"/>
<connect gate="G" pin="A11" pad="K3"/>
<connect gate="G" pin="A12" pad="L3"/>
<connect gate="G" pin="A13" pad="M3"/>
<connect gate="G" pin="A14" pad="K4"/>
<connect gate="G" pin="A15" pad="A8"/>
<connect gate="G" pin="A16" pad="A9"/>
<connect gate="G" pin="A17" pad="A10"/>
<connect gate="G" pin="A18" pad="B10"/>
<connect gate="G" pin="A19" pad="C10"/>
<connect gate="G" pin="A2" pad="M1"/>
<connect gate="G" pin="A20" pad="D10"/>
<connect gate="G" pin="A21" pad="T4"/>
<connect gate="G" pin="A22" pad="R4"/>
<connect gate="G" pin="A23" pad="P4"/>
<connect gate="G" pin="A3" pad="N1"/>
<connect gate="G" pin="A4" pad="P1"/>
<connect gate="G" pin="A5" pad="J2"/>
<connect gate="G" pin="A6" pad="K2"/>
<connect gate="G" pin="A7" pad="L2"/>
<connect gate="G" pin="A8" pad="M2"/>
<connect gate="G" pin="A9" pad="N2"/>
<connect gate="G" pin="AD0" pad="C8"/>
<connect gate="G" pin="AD1" pad="C7"/>
<connect gate="G" pin="AD10" pad="F1"/>
<connect gate="G" pin="AD11" pad="E3"/>
<connect gate="G" pin="AD12" pad="F3"/>
<connect gate="G" pin="AD13" pad="G1"/>
<connect gate="G" pin="AD14" pad="H2"/>
<connect gate="G" pin="AD15" pad="G3"/>
<connect gate="G" pin="AD16" pad="D7"/>
<connect gate="G" pin="AD17" pad="B5"/>
<connect gate="G" pin="AD18" pad="A4"/>
<connect gate="G" pin="AD19" pad="B4"/>
<connect gate="G" pin="AD2" pad="B6"/>
<connect gate="G" pin="AD20" pad="C4"/>
<connect gate="G" pin="AD21" pad="B3"/>
<connect gate="G" pin="AD22" pad="B2"/>
<connect gate="G" pin="AD23" pad="B1"/>
<connect gate="G" pin="AD24" pad="C1"/>
<connect gate="G" pin="AD25" pad="D3"/>
<connect gate="G" pin="AD26" pad="E2"/>
<connect gate="G" pin="AD27" pad="F2"/>
<connect gate="G" pin="AD28" pad="F4"/>
<connect gate="G" pin="AD29" pad="G4"/>
<connect gate="G" pin="AD3" pad="C6"/>
<connect gate="G" pin="AD30" pad="H3"/>
<connect gate="G" pin="AD31" pad="G2"/>
<connect gate="G" pin="AD4" pad="C5"/>
<connect gate="G" pin="AD5" pad="A3"/>
<connect gate="G" pin="AD6" pad="A2"/>
<connect gate="G" pin="AD7" pad="C3"/>
<connect gate="G" pin="AD8" pad="C2"/>
<connect gate="G" pin="AD9" pad="D2"/>
<connect gate="G" pin="ALE" pad="R3"/>
<connect gate="G" pin="BC0" pad="A5"/>
<connect gate="G" pin="BC1" pad="A6"/>
<connect gate="G" pin="BC2" pad="B7"/>
<connect gate="G" pin="BC3" pad="A7"/>
<connect gate="G" pin="BFCLKI" pad="D1"/>
<connect gate="G" pin="BFCLKO" pad="E1"/>
<connect gate="G" pin="CKE" pad="L4"/>
<connect gate="G" pin="CS0" pad="D9"/>
<connect gate="G" pin="CS1" pad="D8"/>
<connect gate="G" pin="CS2" pad="C9"/>
<connect gate="G" pin="CS3" pad="B8"/>
<connect gate="G" pin="D+" pad="T14"/>
<connect gate="G" pin="D-" pad="T15"/>
<connect gate="G" pin="HWCFG0" pad="M14"/>
<connect gate="G" pin="HWCFG1" pad="L14"/>
<connect gate="G" pin="HWCFG2" pad="T6"/>
<connect gate="G" pin="MI_MDIO" pad="R1"/>
<connect gate="G" pin="MI_RXCLK" pad="R2"/>
<connect gate="G" pin="MI_TXCLK" pad="T2"/>
<connect gate="G" pin="NMI" pad="T7"/>
<connect gate="G" pin="P4.0" pad="R8"/>
<connect gate="G" pin="P4.1" pad="R9"/>
<connect gate="G" pin="P4.2" pad="N7"/>
<connect gate="G" pin="P4.3" pad="N6"/>
<connect gate="G" pin="P4.4" pad="P6"/>
<connect gate="G" pin="P4.5" pad="R7"/>
<connect gate="G" pin="P4.6" pad="R6"/>
<connect gate="G" pin="P4.7" pad="P5"/>
<connect gate="G" pin="SDCLKI" pad="J1"/>
<connect gate="G" pin="SDCLKO" pad="H1"/>
<connect gate="G" pin="TCK" pad="T12"/>
<connect gate="G" pin="TDI" pad="T13"/>
<connect gate="G" pin="TDO" pad="T10"/>
<connect gate="G" pin="TMS" pad="T9"/>
<connect gate="G" pin="TRCLK" pad="T8"/>
<connect gate="G" pin="TRST" pad="T11"/>
<connect gate="G" pin="VDDOSC" pad="L16"/>
<connect gate="G" pin="VDDOSC3" pad="P16"/>
<connect gate="G" pin="VSSOSC" pad="N4"/>
<connect gate="G" pin="VSSOSC3" pad="R16"/>
<connect gate="G" pin="XTAL1" pad="M16"/>
<connect gate="G" pin="XTAL2" pad="N16"/>
<connect gate="P0" pin="0" pad="N11"/>
<connect gate="P0" pin="1" pad="P15"/>
<connect gate="P0" pin="10" pad="R14"/>
<connect gate="P0" pin="11" pad="N9"/>
<connect gate="P0" pin="12" pad="P9"/>
<connect gate="P0" pin="13" pad="P8"/>
<connect gate="P0" pin="14" pad="N8"/>
<connect gate="P0" pin="15" pad="P7"/>
<connect gate="P0" pin="2" pad="P10"/>
<connect gate="P0" pin="3" pad="M15"/>
<connect gate="P0" pin="4" pad="R11"/>
<connect gate="P0" pin="5" pad="R12"/>
<connect gate="P0" pin="6" pad="R10"/>
<connect gate="P0" pin="7" pad="N10"/>
<connect gate="P0" pin="8" pad="R13"/>
<connect gate="P0" pin="9" pad="R15"/>
<connect gate="P1" pin="0" pad="D11"/>
<connect gate="P1" pin="1" pad="C12"/>
<connect gate="P1" pin="10" pad="B14"/>
<connect gate="P1" pin="11" pad="C14"/>
<connect gate="P1" pin="12" pad="F13"/>
<connect gate="P1" pin="13" pad="E14"/>
<connect gate="P1" pin="14" pad="D14"/>
<connect gate="P1" pin="15" pad="F14"/>
<connect gate="P1" pin="2" pad="D12"/>
<connect gate="P1" pin="3" pad="B12"/>
<connect gate="P1" pin="4" pad="C11"/>
<connect gate="P1" pin="5" pad="C13"/>
<connect gate="P1" pin="6" pad="A12"/>
<connect gate="P1" pin="7" pad="B13"/>
<connect gate="P1" pin="8" pad="A13"/>
<connect gate="P1" pin="9" pad="A14"/>
<connect gate="P2" pin="0" pad="P12"/>
<connect gate="P2" pin="1" pad="P11"/>
<connect gate="P2" pin="10" pad="L13"/>
<connect gate="P2" pin="11" pad="G16"/>
<connect gate="P2" pin="12" pad="K15"/>
<connect gate="P2" pin="13" pad="K14"/>
<connect gate="P2" pin="14" pad="F16"/>
<connect gate="P2" pin="15" pad="E16"/>
<connect gate="P2" pin="2" pad="P13"/>
<connect gate="P2" pin="3" pad="P14"/>
<connect gate="P2" pin="4" pad="N15"/>
<connect gate="P2" pin="5" pad="N14"/>
<connect gate="P2" pin="6" pad="N12"/>
<connect gate="P2" pin="7" pad="K16"/>
<connect gate="P2" pin="8" pad="J16"/>
<connect gate="P2" pin="9" pad="H16"/>
<connect gate="P3" pin="0" pad="A15"/>
<connect gate="P3" pin="1" pad="B15"/>
<connect gate="P3" pin="10" pad="B16"/>
<connect gate="P3" pin="11" pad="C16"/>
<connect gate="P3" pin="12" pad="D16"/>
<connect gate="P3" pin="13" pad="K13"/>
<connect gate="P3" pin="14" pad="J14"/>
<connect gate="P3" pin="15" pad="J15"/>
<connect gate="P3" pin="2" pad="D15"/>
<connect gate="P3" pin="3" pad="E15"/>
<connect gate="P3" pin="4" pad="G14"/>
<connect gate="P3" pin="5" pad="G15"/>
<connect gate="P3" pin="6" pad="F15"/>
<connect gate="P3" pin="7" pad="H14"/>
<connect gate="P3" pin="8" pad="C15"/>
<connect gate="P3" pin="9" pad="H15"/>
<connect gate="PWR" pin="VDD@0" pad="G7"/>
<connect gate="PWR" pin="VDD@1" pad="G8"/>
<connect gate="PWR" pin="VDD@2" pad="G9"/>
<connect gate="PWR" pin="VDD@3" pad="G10"/>
<connect gate="PWR" pin="VDD@4" pad="G13"/>
<connect gate="PWR" pin="VDD@5" pad="K7"/>
<connect gate="PWR" pin="VDD@6" pad="K8"/>
<connect gate="PWR" pin="VDD@7" pad="K9"/>
<connect gate="PWR" pin="VDD@8" pad="K10"/>
<connect gate="PWR" pin="VDDP@0" pad="D4"/>
<connect gate="PWR" pin="VDDP@1" pad="D13"/>
<connect gate="PWR" pin="VDDP@2" pad="H4"/>
<connect gate="PWR" pin="VDDP@3" pad="J13"/>
<connect gate="PWR" pin="VDDP@4" pad="M4"/>
<connect gate="PWR" pin="VDDP@5" pad="N13"/>
<connect gate="PWR" pin="VSS@0" pad="E4"/>
<connect gate="PWR" pin="VSS@1" pad="E13"/>
<connect gate="PWR" pin="VSS@10" pad="J9"/>
<connect gate="PWR" pin="VSS@11" pad="J10"/>
<connect gate="PWR" pin="VSS@12" pad="L15"/>
<connect gate="PWR" pin="VSS@13" pad="M13"/>
<connect gate="PWR" pin="VSS@2" pad="H7"/>
<connect gate="PWR" pin="VSS@3" pad="H8"/>
<connect gate="PWR" pin="VSS@4" pad="H9"/>
<connect gate="PWR" pin="VSS@5" pad="H10"/>
<connect gate="PWR" pin="VSS@6" pad="H13"/>
<connect gate="PWR" pin="VSS@7" pad="J4"/>
<connect gate="PWR" pin="VSS@8" pad="J7"/>
<connect gate="PWR" pin="VSS@9" pad="J8"/>
<connect gate="RES" pin="RESERVED@0" pad="A1"/>
<connect gate="RES" pin="RESERVED@1" pad="A16"/>
<connect gate="RES" pin="RESERVED@2" pad="T1"/>
<connect gate="RES" pin="RESERVED@3" pad="T16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1100" prefix="IC">
<description>&lt;b&gt;32-bit Consumer Class TriCore&lt;/b&gt; Single-Chip Microcontroller&lt;p&gt;
Source: http://www.infineon.com/cmc_upload/documents/010/9915/TC1100_umsu_v10.pdf</description>
<gates>
<gate name="-C" symbol="TC1100"/>
<gate name="-P0" symbol="PORT16"/>
<gate name="-P1" symbol="PORT16"/>
<gate name="-P2" symbol="PORT16"/>
<gate name="-P3" symbol="PORT16"/>
<gate name="-P4" symbol="PORT8"/>
<gate name="-AD" symbol="AD31"/>
<gate name="-A" symbol="A23"/>
<gate name="-JTAG" symbol="JTAG"/>
<gate name="-VSS1" symbol="VSS"/>
<gate name="-VSS2" symbol="VSS"/>
<gate name="-VSS3" symbol="VSS"/>
<gate name="-VSS4" symbol="VSS"/>
<gate name="-VSS5" symbol="VSS"/>
<gate name="-VSS6" symbol="VSS"/>
<gate name="-VSS7" symbol="VSS"/>
<gate name="-VSS8" symbol="VSS"/>
<gate name="-VSS9" symbol="VSS"/>
<gate name="-VSS10" symbol="VSS"/>
<gate name="-VSS11" symbol="VSS"/>
<gate name="-VSS12" symbol="VSS"/>
<gate name="-VSS13" symbol="VSS"/>
<gate name="-VSS14" symbol="VSS"/>
<gate name="-VSS15" symbol="VSS"/>
<gate name="-VSS16" symbol="VSS"/>
<gate name="-VDD1" symbol="VDD"/>
<gate name="-VDD2" symbol="VDD"/>
<gate name="-VDD3" symbol="VDD"/>
<gate name="-VDD4" symbol="VDD"/>
<gate name="-VDD5" symbol="VDD"/>
<gate name="-VDD6" symbol="VDD"/>
<gate name="-VDD7" symbol="VDD"/>
<gate name="-VDD8" symbol="VDD"/>
<gate name="-VDD9" symbol="VDD"/>
<gate name="-VDDP1" symbol="VDDP"/>
<gate name="-VDDP2" symbol="VDDP"/>
<gate name="-VDDP3" symbol="VDDP"/>
<gate name="-VDDP4" symbol="VDDP"/>
<gate name="-VDDP5" symbol="VDDP"/>
<gate name="-VDDP6" symbol="VDDP"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="-A" pin="A0" pad="K1"/>
<connect gate="-A" pin="A1" pad="L1"/>
<connect gate="-A" pin="A10" pad="J3"/>
<connect gate="-A" pin="A11" pad="K3"/>
<connect gate="-A" pin="A12" pad="L3"/>
<connect gate="-A" pin="A13" pad="M3"/>
<connect gate="-A" pin="A14" pad="K4"/>
<connect gate="-A" pin="A15" pad="A8"/>
<connect gate="-A" pin="A16" pad="A9"/>
<connect gate="-A" pin="A17" pad="A10"/>
<connect gate="-A" pin="A18" pad="B10"/>
<connect gate="-A" pin="A19" pad="C10"/>
<connect gate="-A" pin="A2" pad="M1"/>
<connect gate="-A" pin="A20" pad="D10"/>
<connect gate="-A" pin="A21" pad="T4"/>
<connect gate="-A" pin="A22" pad="R4"/>
<connect gate="-A" pin="A23" pad="P4"/>
<connect gate="-A" pin="A3" pad="N1"/>
<connect gate="-A" pin="A4" pad="P1"/>
<connect gate="-A" pin="A5" pad="J2"/>
<connect gate="-A" pin="A6" pad="K2"/>
<connect gate="-A" pin="A7" pad="L2"/>
<connect gate="-A" pin="A8" pad="M2"/>
<connect gate="-A" pin="A9" pad="N2"/>
<connect gate="-AD" pin="AD0" pad="C8"/>
<connect gate="-AD" pin="AD1" pad="C7"/>
<connect gate="-AD" pin="AD10" pad="F1"/>
<connect gate="-AD" pin="AD11" pad="E3"/>
<connect gate="-AD" pin="AD12" pad="F3"/>
<connect gate="-AD" pin="AD13" pad="G1"/>
<connect gate="-AD" pin="AD14" pad="H2"/>
<connect gate="-AD" pin="AD15" pad="G3"/>
<connect gate="-AD" pin="AD16" pad="D7"/>
<connect gate="-AD" pin="AD17" pad="B5"/>
<connect gate="-AD" pin="AD18" pad="A4"/>
<connect gate="-AD" pin="AD19" pad="B4"/>
<connect gate="-AD" pin="AD2" pad="B6"/>
<connect gate="-AD" pin="AD20" pad="C4"/>
<connect gate="-AD" pin="AD21" pad="B3"/>
<connect gate="-AD" pin="AD22" pad="B2"/>
<connect gate="-AD" pin="AD23" pad="B1"/>
<connect gate="-AD" pin="AD24" pad="C1"/>
<connect gate="-AD" pin="AD25" pad="D3"/>
<connect gate="-AD" pin="AD26" pad="E2"/>
<connect gate="-AD" pin="AD27" pad="F2"/>
<connect gate="-AD" pin="AD28" pad="F4"/>
<connect gate="-AD" pin="AD29" pad="G4"/>
<connect gate="-AD" pin="AD3" pad="C6"/>
<connect gate="-AD" pin="AD30" pad="H3"/>
<connect gate="-AD" pin="AD31" pad="G2"/>
<connect gate="-AD" pin="AD4" pad="C5"/>
<connect gate="-AD" pin="AD5" pad="A3"/>
<connect gate="-AD" pin="AD6" pad="A2"/>
<connect gate="-AD" pin="AD7" pad="C3"/>
<connect gate="-AD" pin="AD8" pad="C2"/>
<connect gate="-AD" pin="AD9" pad="D2"/>
<connect gate="-C" pin="!ADV" pad="B11"/>
<connect gate="-C" pin="!BAA" pad="A11"/>
<connect gate="-C" pin="!BC0" pad="A5"/>
<connect gate="-C" pin="!BC1" pad="A6"/>
<connect gate="-C" pin="!BC2" pad="B7"/>
<connect gate="-C" pin="!BC3" pad="A7"/>
<connect gate="-C" pin="!BRKIN" pad="T5"/>
<connect gate="-C" pin="!CAS" pad="D5"/>
<connect gate="-C" pin="!CS0" pad="D9"/>
<connect gate="-C" pin="!CS1" pad="D8"/>
<connect gate="-C" pin="!CS2" pad="C9"/>
<connect gate="-C" pin="!CS3" pad="B8"/>
<connect gate="-C" pin="!CSCOMB" pad="N3"/>
<connect gate="-C" pin="!HDRST" pad="N5"/>
<connect gate="-C" pin="!MR_W" pad="P3"/>
<connect gate="-C" pin="!NMI" pad="T7"/>
<connect gate="-C" pin="!PORST" pad="R5"/>
<connect gate="-C" pin="!RAS" pad="D6"/>
<connect gate="-C" pin="!RD" pad="P2"/>
<connect gate="-C" pin="!RD_WR" pad="T3"/>
<connect gate="-C" pin="!TRCLK" pad="T8"/>
<connect gate="-C" pin="!WAIT" pad="B9"/>
<connect gate="-C" pin="ALE" pad="R3"/>
<connect gate="-C" pin="BFCLKI" pad="D1"/>
<connect gate="-C" pin="BFCLKO" pad="E1"/>
<connect gate="-C" pin="CKE" pad="L4"/>
<connect gate="-C" pin="HWCFG0" pad="M14"/>
<connect gate="-C" pin="HWCFG1" pad="L14"/>
<connect gate="-C" pin="HWCFG2" pad="T6"/>
<connect gate="-C" pin="NC@1" pad="R1"/>
<connect gate="-C" pin="NC@2" pad="T14"/>
<connect gate="-C" pin="NC@3" pad="T15"/>
<connect gate="-C" pin="RESERVED@1" pad="A1"/>
<connect gate="-C" pin="RESERVED@2" pad="A16"/>
<connect gate="-C" pin="RESERVED@3" pad="T1"/>
<connect gate="-C" pin="RESERVED@4" pad="T16"/>
<connect gate="-C" pin="SDCLKI" pad="J1"/>
<connect gate="-C" pin="SDCLKO" pad="H1"/>
<connect gate="-C" pin="VDDOSC" pad="L16"/>
<connect gate="-C" pin="VDDOSC3" pad="P16"/>
<connect gate="-C" pin="VSSOSC" pad="L15"/>
<connect gate="-C" pin="VSSOSC3" pad="R16"/>
<connect gate="-C" pin="XTAL1" pad="M16"/>
<connect gate="-C" pin="XTAL2" pad="N16"/>
<connect gate="-JTAG" pin="!TRST" pad="T11"/>
<connect gate="-JTAG" pin="TCK" pad="T12"/>
<connect gate="-JTAG" pin="TDI" pad="T13"/>
<connect gate="-JTAG" pin="TDO" pad="T10"/>
<connect gate="-JTAG" pin="TMS" pad="T9"/>
<connect gate="-P0" pin="0" pad="N11"/>
<connect gate="-P0" pin="1" pad="P15"/>
<connect gate="-P0" pin="10" pad="R14"/>
<connect gate="-P0" pin="11" pad="N9"/>
<connect gate="-P0" pin="12" pad="P9"/>
<connect gate="-P0" pin="13" pad="P8"/>
<connect gate="-P0" pin="14" pad="N8"/>
<connect gate="-P0" pin="15" pad="P7"/>
<connect gate="-P0" pin="2" pad="P10"/>
<connect gate="-P0" pin="3" pad="M15"/>
<connect gate="-P0" pin="4" pad="R11"/>
<connect gate="-P0" pin="5" pad="R12"/>
<connect gate="-P0" pin="6" pad="R10"/>
<connect gate="-P0" pin="7" pad="N10"/>
<connect gate="-P0" pin="8" pad="R13"/>
<connect gate="-P0" pin="9" pad="R15"/>
<connect gate="-P1" pin="0" pad="D11"/>
<connect gate="-P1" pin="1" pad="C12"/>
<connect gate="-P1" pin="10" pad="B14"/>
<connect gate="-P1" pin="11" pad="C14"/>
<connect gate="-P1" pin="12" pad="F13"/>
<connect gate="-P1" pin="13" pad="E14"/>
<connect gate="-P1" pin="14" pad="D14"/>
<connect gate="-P1" pin="15" pad="F14"/>
<connect gate="-P1" pin="2" pad="D12"/>
<connect gate="-P1" pin="3" pad="B12"/>
<connect gate="-P1" pin="4" pad="C11"/>
<connect gate="-P1" pin="5" pad="C13"/>
<connect gate="-P1" pin="6" pad="A12"/>
<connect gate="-P1" pin="7" pad="B13"/>
<connect gate="-P1" pin="8" pad="A13"/>
<connect gate="-P1" pin="9" pad="A14"/>
<connect gate="-P2" pin="0" pad="P12"/>
<connect gate="-P2" pin="1" pad="P11"/>
<connect gate="-P2" pin="10" pad="L13"/>
<connect gate="-P2" pin="11" pad="G16"/>
<connect gate="-P2" pin="12" pad="K15"/>
<connect gate="-P2" pin="13" pad="K14"/>
<connect gate="-P2" pin="14" pad="F16"/>
<connect gate="-P2" pin="15" pad="E16"/>
<connect gate="-P2" pin="2" pad="P13"/>
<connect gate="-P2" pin="3" pad="P14"/>
<connect gate="-P2" pin="4" pad="N15"/>
<connect gate="-P2" pin="5" pad="N14"/>
<connect gate="-P2" pin="6" pad="N12"/>
<connect gate="-P2" pin="7" pad="K16"/>
<connect gate="-P2" pin="8" pad="J16"/>
<connect gate="-P2" pin="9" pad="H16"/>
<connect gate="-P3" pin="0" pad="A15"/>
<connect gate="-P3" pin="1" pad="B15"/>
<connect gate="-P3" pin="10" pad="B16"/>
<connect gate="-P3" pin="11" pad="C16"/>
<connect gate="-P3" pin="12" pad="D16"/>
<connect gate="-P3" pin="13" pad="K13"/>
<connect gate="-P3" pin="14" pad="J14"/>
<connect gate="-P3" pin="15" pad="J15"/>
<connect gate="-P3" pin="2" pad="D15"/>
<connect gate="-P3" pin="3" pad="E15"/>
<connect gate="-P3" pin="4" pad="G14"/>
<connect gate="-P3" pin="5" pad="G15"/>
<connect gate="-P3" pin="6" pad="F15"/>
<connect gate="-P3" pin="7" pad="H14"/>
<connect gate="-P3" pin="8" pad="C15"/>
<connect gate="-P3" pin="9" pad="H15"/>
<connect gate="-P4" pin="0" pad="R8"/>
<connect gate="-P4" pin="1" pad="R9"/>
<connect gate="-P4" pin="2" pad="N7"/>
<connect gate="-P4" pin="3" pad="N6"/>
<connect gate="-P4" pin="4" pad="P6"/>
<connect gate="-P4" pin="5" pad="R7"/>
<connect gate="-P4" pin="6" pad="R6"/>
<connect gate="-P4" pin="7" pad="P5"/>
<connect gate="-VDD1" pin="VDD" pad="G7"/>
<connect gate="-VDD2" pin="VDD" pad="G8"/>
<connect gate="-VDD3" pin="VDD" pad="G9"/>
<connect gate="-VDD4" pin="VDD" pad="G10"/>
<connect gate="-VDD5" pin="VDD" pad="G13"/>
<connect gate="-VDD6" pin="VDD" pad="K7"/>
<connect gate="-VDD7" pin="VDD" pad="K8"/>
<connect gate="-VDD8" pin="VDD" pad="K9"/>
<connect gate="-VDD9" pin="VDD" pad="K10"/>
<connect gate="-VDDP1" pin="VDDP" pad="D4"/>
<connect gate="-VDDP2" pin="VDDP" pad="D13"/>
<connect gate="-VDDP3" pin="VDDP" pad="H4"/>
<connect gate="-VDDP4" pin="VDDP" pad="J13"/>
<connect gate="-VDDP5" pin="VDDP" pad="M4"/>
<connect gate="-VDDP6" pin="VDDP" pad="N13"/>
<connect gate="-VSS1" pin="VSS" pad="E4"/>
<connect gate="-VSS10" pin="VSS" pad="J8"/>
<connect gate="-VSS11" pin="VSS" pad="J9"/>
<connect gate="-VSS12" pin="VSS" pad="J10"/>
<connect gate="-VSS13" pin="VSS" pad="M13"/>
<connect gate="-VSS14" pin="VSS" pad="N4"/>
<connect gate="-VSS15" pin="VSS" pad="R2"/>
<connect gate="-VSS16" pin="VSS" pad="T2"/>
<connect gate="-VSS2" pin="VSS" pad="E13"/>
<connect gate="-VSS3" pin="VSS" pad="H7"/>
<connect gate="-VSS4" pin="VSS" pad="H8"/>
<connect gate="-VSS5" pin="VSS" pad="H9"/>
<connect gate="-VSS6" pin="VSS" pad="H10"/>
<connect gate="-VSS7" pin="VSS" pad="H13"/>
<connect gate="-VSS8" pin="VSS" pad="J4"/>
<connect gate="-VSS9" pin="VSS" pad="J7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC191*" prefix="IC">
<description>&lt;b&gt;32 bit TriCore based microcontroller/DSP&lt;/b&gt;&lt;p&gt;
 which is mainly designed for automotive telematics applications.&lt;br&gt;
Source: http://www.infineon.com .. TC1910_DS_V1.0.pdf / TC1912_DS_V1.0.pdf</description>
<gates>
<gate name="-C" symbol="TC1910"/>
<gate name="-JTAG" symbol="JTAG-OCSD"/>
<gate name="-P0" symbol="PORT0-10_12"/>
<gate name="-P1" symbol="PORT1-10_12"/>
<gate name="-P2" symbol="PORT2-10_12"/>
<gate name="-P3" symbol="PORT3-10_12"/>
<gate name="HS1" symbol="HEATSINK"/>
<gate name="HS2" symbol="HEATSINK"/>
<gate name="HS3" symbol="HEATSINK"/>
<gate name="HS4" symbol="HEATSINK"/>
<gate name="HS5" symbol="HEATSINK"/>
<gate name="HS6" symbol="HEATSINK"/>
<gate name="HS7" symbol="HEATSINK"/>
<gate name="HS8" symbol="HEATSINK"/>
<gate name="HS9" symbol="HEATSINK"/>
<gate name="HS10" symbol="HEATSINK"/>
<gate name="HS11" symbol="HEATSINK"/>
<gate name="HS12" symbol="HEATSINK"/>
<gate name="HS13" symbol="HEATSINK"/>
<gate name="HS14" symbol="HEATSINK"/>
<gate name="HS15" symbol="HEATSINK"/>
<gate name="HS0" symbol="HEATSINK"/>
<gate name="-A" symbol="A23"/>
<gate name="-AD" symbol="AD31"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="-A" pin="A0" pad="R3"/>
<connect gate="-A" pin="A1" pad="P4"/>
<connect gate="-A" pin="A10" pad="N1"/>
<connect gate="-A" pin="A11" pad="M4"/>
<connect gate="-A" pin="A12" pad="M3"/>
<connect gate="-A" pin="A13" pad="L4"/>
<connect gate="-A" pin="A14" pad="M2"/>
<connect gate="-A" pin="A15" pad="M1"/>
<connect gate="-A" pin="A16" pad="L3"/>
<connect gate="-A" pin="A17" pad="L1"/>
<connect gate="-A" pin="A18" pad="L2"/>
<connect gate="-A" pin="A19" pad="K4"/>
<connect gate="-A" pin="A2" pad="T1"/>
<connect gate="-A" pin="A20" pad="K3"/>
<connect gate="-A" pin="A21" pad="J4"/>
<connect gate="-A" pin="A22" pad="K2"/>
<connect gate="-A" pin="A23" pad="J3"/>
<connect gate="-A" pin="A3" pad="R2"/>
<connect gate="-A" pin="A4" pad="R1"/>
<connect gate="-A" pin="A5" pad="P3"/>
<connect gate="-A" pin="A6" pad="P2"/>
<connect gate="-A" pin="A7" pad="P1"/>
<connect gate="-A" pin="A8" pad="N3"/>
<connect gate="-A" pin="A9" pad="N2"/>
<connect gate="-AD" pin="AD0" pad="H4"/>
<connect gate="-AD" pin="AD1" pad="J2"/>
<connect gate="-AD" pin="AD10" pad="G3"/>
<connect gate="-AD" pin="AD11" pad="G2"/>
<connect gate="-AD" pin="AD12" pad="F4"/>
<connect gate="-AD" pin="AD13" pad="C1"/>
<connect gate="-AD" pin="AD14" pad="F3"/>
<connect gate="-AD" pin="AD15" pad="F2"/>
<connect gate="-AD" pin="AD16" pad="E3"/>
<connect gate="-AD" pin="AD17" pad="B1"/>
<connect gate="-AD" pin="AD18" pad="E2"/>
<connect gate="-AD" pin="AD19" pad="E4"/>
<connect gate="-AD" pin="AD2" pad="H1"/>
<connect gate="-AD" pin="AD20" pad="A1"/>
<connect gate="-AD" pin="AD21" pad="D2"/>
<connect gate="-AD" pin="AD22" pad="D3"/>
<connect gate="-AD" pin="AD23" pad="C2"/>
<connect gate="-AD" pin="AD24" pad="C3"/>
<connect gate="-AD" pin="AD25" pad="B2"/>
<connect gate="-AD" pin="AD26" pad="A2"/>
<connect gate="-AD" pin="AD27" pad="B3"/>
<connect gate="-AD" pin="AD28" pad="A3"/>
<connect gate="-AD" pin="AD29" pad="A4"/>
<connect gate="-AD" pin="AD3" pad="H3"/>
<connect gate="-AD" pin="AD30" pad="B4"/>
<connect gate="-AD" pin="AD31" pad="C4"/>
<connect gate="-AD" pin="AD4" pad="H2"/>
<connect gate="-AD" pin="AD5" pad="G1"/>
<connect gate="-AD" pin="AD6" pad="G4"/>
<connect gate="-AD" pin="AD7" pad="F1"/>
<connect gate="-AD" pin="AD8" pad="E1"/>
<connect gate="-AD" pin="AD9" pad="D1"/>
<connect gate="-C" pin="!ADV" pad="N9"/>
<connect gate="-C" pin="!BAA" pad="P8"/>
<connect gate="-C" pin="!BC0" pad="N6"/>
<connect gate="-C" pin="!BC1" pad="R5"/>
<connect gate="-C" pin="!BC2" pad="T4"/>
<connect gate="-C" pin="!BC3" pad="T3"/>
<connect gate="-C" pin="!CAS" pad="T2"/>
<connect gate="-C" pin="!CMDELAY" pad="T9"/>
<connect gate="-C" pin="!CS0" pad="R7"/>
<connect gate="-C" pin="!CS1" pad="N7"/>
<connect gate="-C" pin="!CS2" pad="P7"/>
<connect gate="-C" pin="!CS3" pad="T6"/>
<connect gate="-C" pin="!CS4" pad="R6"/>
<connect gate="-C" pin="!CS5" pad="T5"/>
<connect gate="-C" pin="!CS6" pad="P6"/>
<connect gate="-C" pin="!CSEMU" pad="R8"/>
<connect gate="-C" pin="!CSGLB" pad="N8"/>
<connect gate="-C" pin="!CSOVL" pad="T8"/>
<connect gate="-C" pin="!HRST" pad="B13"/>
<connect gate="-C" pin="!MR_W" pad="R9"/>
<connect gate="-C" pin="!NMI" pad="A13"/>
<connect gate="-C" pin="!PORST" pad="C13"/>
<connect gate="-C" pin="!RAS" pad="N5"/>
<connect gate="-C" pin="!RD" pad="R4"/>
<connect gate="-C" pin="!RD_WR" pad="P5"/>
<connect gate="-C" pin="!SCANMODE" pad="J14"/>
<connect gate="-C" pin="!WAIT" pad="T7"/>
<connect gate="-C" pin="AI0+" pad="D9"/>
<connect gate="-C" pin="AI0-" pad="B9"/>
<connect gate="-C" pin="AI1+" pad="C10"/>
<connect gate="-C" pin="AI1-" pad="B10"/>
<connect gate="-C" pin="ALE" pad="R10"/>
<connect gate="-C" pin="AO0+" pad="C11"/>
<connect gate="-C" pin="AO0-" pad="B12"/>
<connect gate="-C" pin="AO1+" pad="B11"/>
<connect gate="-C" pin="AO1-" pad="D11"/>
<connect gate="-C" pin="BFCLK0" pad="K1"/>
<connect gate="-C" pin="BYPASS" pad="A12"/>
<connect gate="-C" pin="CEXT" pad="D12"/>
<connect gate="-C" pin="CKE" pad="P9"/>
<connect gate="-C" pin="CLKOUT" pad="A14"/>
<connect gate="-C" pin="CODEC_DIS" pad="C12"/>
<connect gate="-C" pin="EBUCLK" pad="J1"/>
<connect gate="-C" pin="PLLCTRL_AO" pad="D8"/>
<connect gate="-C" pin="TM_CTRL0" pad="C7"/>
<connect gate="-C" pin="TM_CTRL1" pad="C5"/>
<connect gate="-C" pin="VAGND_GOD" pad="C9"/>
<connect gate="-C" pin="VAREF_GOD" pad="D10"/>
<connect gate="-C" pin="VDDPLL" pad="B6"/>
<connect gate="-C" pin="VDDR" pad="D6"/>
<connect gate="-C" pin="VDDSB" pad="L13"/>
<connect gate="-C" pin="VDD_COD0/1" pad="A10"/>
<connect gate="-C" pin="VDD_GUARD" pad="B8"/>
<connect gate="-C" pin="VDD_OSCI" pad="D7"/>
<connect gate="-C" pin="VDD_PLL" pad="A9"/>
<connect gate="-C" pin="VDD_PWR2@1" pad="G7"/>
<connect gate="-C" pin="VDD_PWR2@2" pad="G10"/>
<connect gate="-C" pin="VDD_PWR2@3" pad="K7"/>
<connect gate="-C" pin="VDD_PWR2@4" pad="K10"/>
<connect gate="-C" pin="VDD_PWR@1" pad="D4"/>
<connect gate="-C" pin="VDD_PWR@2" pad="D13"/>
<connect gate="-C" pin="VDD_PWR@3" pad="H7"/>
<connect gate="-C" pin="VDD_PWR@4" pad="N4"/>
<connect gate="-C" pin="VDD_PWR@5" pad="N13"/>
<connect gate="-C" pin="VDD_RTC" pad="A5"/>
<connect gate="-C" pin="VSSA_COD0/1" pad="A11"/>
<connect gate="-C" pin="VSSPLL" pad="A8"/>
<connect gate="-C" pin="VSS_32K" pad="B5"/>
<connect gate="-C" pin="VSS_GND@1" pad="G8"/>
<connect gate="-C" pin="VSS_GND@2" pad="G9"/>
<connect gate="-C" pin="VSS_GND@3" pad="H8"/>
<connect gate="-C" pin="VSS_GND@4" pad="H9"/>
<connect gate="-C" pin="VSS_GND@5" pad="J8"/>
<connect gate="-C" pin="VSS_GND@6" pad="J9"/>
<connect gate="-C" pin="VSS_GUARD" pad="C8"/>
<connect gate="-C" pin="VSS_PLL" pad="B7"/>
<connect gate="-C" pin="XTAL1" pad="A6"/>
<connect gate="-C" pin="XTAL2" pad="A7"/>
<connect gate="-C" pin="XTAL3" pad="D5"/>
<connect gate="-C" pin="XTAL4" pad="C6"/>
<connect gate="-JTAG" pin="!BRKIN" pad="R13"/>
<connect gate="-JTAG" pin="!BRKOUT" pad="P12"/>
<connect gate="-JTAG" pin="!OCDSE" pad="T14"/>
<connect gate="-JTAG" pin="!TRST" pad="T16"/>
<connect gate="-JTAG" pin="TCK" pad="R15"/>
<connect gate="-JTAG" pin="TDI" pad="T15"/>
<connect gate="-JTAG" pin="TDO" pad="R14"/>
<connect gate="-JTAG" pin="TMS" pad="P13"/>
<connect gate="-P0" pin="0/EXI0IN" pad="M14"/>
<connect gate="-P0" pin="1/EXI1IN/DATA_IN" pad="M15"/>
<connect gate="-P0" pin="2/EXI2IN/DATA_OUT" pad="M16"/>
<connect gate="-P0" pin="3/EXI3IN/MCLK" pad="L14"/>
<connect gate="-P0" pin="4/GPIO/SCLK" pad="L15"/>
<connect gate="-P0" pin="5/GPIO/LRCK" pad="K13"/>
<connect gate="-P0" pin="6/GPIO/MUTE0" pad="L16"/>
<connect gate="-P0" pin="7/GPIO/MUTE1" pad="K14"/>
<connect gate="-P1" pin="0/GPIO" pad="P14"/>
<connect gate="-P1" pin="1/GPIO" pad="R16"/>
<connect gate="-P1" pin="2/GPIO" pad="P15"/>
<connect gate="-P1" pin="3/GPIO" pad="P16"/>
<connect gate="-P1" pin="4/GPIO" pad="N14"/>
<connect gate="-P1" pin="5/GPIO" pad="N15"/>
<connect gate="-P1" pin="6/GPIO" pad="N16"/>
<connect gate="-P1" pin="7/GPIO" pad="M13"/>
<connect gate="-P2" pin="0/GPIO/RXDCAN0" pad="A16"/>
<connect gate="-P2" pin="1/GPIO/TXDCAN0" pad="G13"/>
<connect gate="-P2" pin="10/RXD0" pad="D15"/>
<connect gate="-P2" pin="11/TXD0" pad="E14"/>
<connect gate="-P2" pin="12/SCLK" pad="D14"/>
<connect gate="-P2" pin="13/MRST" pad="E13"/>
<connect gate="-P2" pin="14/MTSR" pad="C14"/>
<connect gate="-P2" pin="15/GPIO/EXI4IN/PLL_CLC.LOCK" pad="B14"/>
<connect gate="-P2" pin="2/GPIO/RXDCAN1" pad="G14"/>
<connect gate="-P2" pin="3/GPIO/TXDCAN1" pad="A15"/>
<connect gate="-P2" pin="4/GPIO" pad="F15"/>
<connect gate="-P2" pin="5/GPIO" pad="B15"/>
<connect gate="-P2" pin="6/SCL" pad="E15"/>
<connect gate="-P2" pin="7/SDA" pad="C15"/>
<connect gate="-P2" pin="8/GPIO" pad="F13"/>
<connect gate="-P2" pin="9/GPIO" pad="F14"/>
<connect gate="-P3" pin="0/GPTU.0" pad="J13"/>
<connect gate="-P3" pin="1/GPTU.1" pad="K16"/>
<connect gate="-P3" pin="10/GPIO/RXD2" pad="G16"/>
<connect gate="-P3" pin="11/GPIO/OSCBYP/TXD2" pad="E16"/>
<connect gate="-P3" pin="12/EXI5IN/HWCFG0" pad="F16"/>
<connect gate="-P3" pin="13/EXI6IN/HWCFG1" pad="G15"/>
<connect gate="-P3" pin="14/EXI7IN/HWCFG2" pad="C16"/>
<connect gate="-P3" pin="15/GPIO" pad="B16"/>
<connect gate="-P3" pin="2/GPTU.2" pad="K15"/>
<connect gate="-P3" pin="3/GPTU.3" pad="J16"/>
<connect gate="-P3" pin="4/GPTU.4" pad="H13"/>
<connect gate="-P3" pin="5/GPTU.5" pad="H14"/>
<connect gate="-P3" pin="6/GPTU.6" pad="J15"/>
<connect gate="-P3" pin="7/GPTU.7" pad="H15"/>
<connect gate="-P3" pin="8/RXD1" pad="H16"/>
<connect gate="-P3" pin="9/TXD1" pad="D16"/>
<connect gate="HS0" pin="HS" pad="N12"/>
<connect gate="HS1" pin="HS" pad="T13"/>
<connect gate="HS10" pin="HS" pad="P10"/>
<connect gate="HS11" pin="HS" pad="N10"/>
<connect gate="HS12" pin="HS" pad="T10"/>
<connect gate="HS13" pin="HS" pad="K9"/>
<connect gate="HS14" pin="HS" pad="K8"/>
<connect gate="HS15" pin="HS" pad="J7"/>
<connect gate="HS2" pin="HS" pad="R12"/>
<connect gate="HS3" pin="HS" pad="T12"/>
<connect gate="HS4" pin="HS" pad="J10"/>
<connect gate="HS5" pin="HS" pad="H10"/>
<connect gate="HS6" pin="HS" pad="P11"/>
<connect gate="HS7" pin="HS" pad="N11"/>
<connect gate="HS8" pin="HS" pad="R11"/>
<connect gate="HS9" pin="HS" pad="T11"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
