<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<library>
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LD260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, square, Siemens</description>
</package>
<package name="LB10">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
10-LED bar graph, DIL, Siemens</description>
</package>
<package name="U57X32">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
rectangle, 5.7 x 3.2 mm</description>
</package>
<package name="LED2X5">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
2 x 5 mm, rectangle</description>
</package>
<package name="DUOLED5MM">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;p&gt;
2 colors, 5 mm, round</description>
</package>
<package name="DUOLED2X5">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;p&gt;
2 colors, 2.5 x 5 mm, recangle</description>
</package>
<package name="LSU260">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
1 mm, round, Siemens</description>
</package>
<package name="LZR181">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
1 LED, Siemens</description>
</package>
<package name="LZR182">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
2 LEDs, Siemens</description>
</package>
<package name="LZR183">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
3 LEDs, Siemens</description>
</package>
<package name="LZR184">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
4 LEDs, Siemens</description>
</package>
<package name="LZR185">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
5 LEDs, Siemens</description>
</package>
<package name="Q62902-B152">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B153">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B155">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="Q62902-B156">
<description>&lt;b&gt;LED HOLDER&lt;/b&gt;&lt;p&gt;
Siemens</description>
</package>
<package name="LD266">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
6 LEDs, Siemens</description>
</package>
<package name="LD269">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
9 LEDs, Siemens</description>
</package>
<package name="SFH480">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="SFH482">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon
TO-18, lead spacing 2.54 mm, cathode marking&lt;p&gt;
Inifineon</description>
</package>
<package name="IRL80A">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
IR transmitter Siemens</description>
</package>
<package name="1206">
<description>&lt;b&gt;CHICAGO MINIATURE LAMP, INC.&lt;/b&gt;&lt;p&gt;
7022X Series SMT LEDs 1206 Package Size</description>
</package>
<package name="P-LCC-2">
<description>&lt;b&gt;TOPLED® High-optical Power LED (HOP)&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... ls_t675.pdf</description>
</package>
<package name="OSRAM-MINI-TOP-LED">
<description>&lt;b&gt;BLUE LINETM Hyper Mini TOPLED® Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LB M676.pdf</description>
</package>
<package name="P-LCC-4">
<description>&lt;b&gt;Power TOPLED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LA_LY E67B.pdf</description>
</package>
<package name="P-LCC-4/2">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LOG_LSG T671.pdf</description>
</package>
<package name="P-LCC-4-2">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LSG T677.pdf</description>
</package>
<package name="OSRAM-SIDELED">
<description>&lt;b&gt;Super SIDELED® High-Current LED&lt;/b&gt;&lt;p&gt;
LG A672, LP A672 &lt;br&gt;
Source: http://www.osram.convergy.de/ ... LG_LP_A672.pdf (2004.05.13)</description>
</package>
<package name="P-LCC-4-3">
<description>&lt;b&gt;Hyper TOPLED® &lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
</package>
<package name="SMART-LED">
<description>&lt;b&gt;SmartLEDTM Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY L896.pdf</description>
</package>
<package name="P-LCC-2-TOPLED-RG">
<description>&lt;b&gt;Hyper TOPLED® RG Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY T776.pdf</description>
</package>
<package name="MICRO-SIDELED">
<description>&lt;b&gt;Hyper Micro SIDELED®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LA_LO_LS_LY Y876.pdf</description>
</package>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="MINI-TOPLED-SANTANA">
<description>&lt;b&gt;Mini TOPLED Santana®&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG M470.pdf</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
<package name="CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="SMARTLED-TTW">
<description>&lt;b&gt;SmartLED TTW&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="PLCC4-TOPLED-RG">
<description>&lt;b&gt;Multi TOPLED® RG&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de ... LSG T770.pdf</description>
</package>
<package name="MSA5XXX">
<description>&lt;b&gt;16 Segment, Single Digit Alpha-Numeric Display&lt;/b&gt; 0.5 Inch (12.7 mm)&lt;p&gt;
Source: www.fairchildsemi.com/ds/MS/MSA5480C.pdf</description>
</package>
<package name="SA08">
<description>&lt;b&gt;Single Digit Numeric Display&lt;/b&gt; 20mm (0.8 Inch)&lt;p&gt;
Source: Kingbright .. SA08-11SRWA.pdf</description>
</package>
<package name="FX08">
<description>&lt;b&gt;Single Digit Numeric Display&lt;/b&gt; 20mm (0.8 Inch)&lt;p&gt;
Source: Kingbright .. SA08-11SRWA.pdf</description>
</package>
<package name="SA08-21">
<description>&lt;b&gt;Single Digit Numeric Display&lt;/b&gt; 20mm (0.8 Inch)&lt;p&gt;
Source: Kingbright .. SA08-11SRWA.pdf</description>
</package>
<package name="SUPERFLUX-7.6X7.6">
<description>&lt;b&gt;SUPER FLUX LED LAMP&lt;/b&gt; 7.6 mm x 7.6 mm &lt;p&gt;
Source: www.us.kingbright.com/images/catalog/SPEC/W7676CPBC-H.pdf</description>
</package>
<package name="SUPERFLUX-SMD-7.6X7.6">
<description>&lt;b&gt;SMD SUPER FLUX LED LAMP&lt;/b&gt; 7.6 mm x 7.6 mm &lt;p&gt;
Source: www.us.kingbright.com/images/catalog/SPEC/W7676CPBC-H05.pdf</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="LUMILED+">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; with cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="LUMILED">
<description>&lt;b&gt;Lumileds Lighting. LUXEON®&lt;/b&gt; without cool pad&lt;p&gt;
Source: K2.pdf</description>
</package>
<package name="SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
<package name="SML0805">
<description>&lt;b&gt;SML0805-2CW-TR (0805 PROFILE)&lt;/b&gt; COOL WHITE&lt;p&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0093.pdf</description>
</package>
<package name="SML1206">
<description>&lt;b&gt;SML10XXKH-TR (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;SML10R3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10E3KH-TR&lt;/td&gt;&lt;td&gt;SUPER REDSUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10O3KH-TR&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PY3KH-TR&lt;/td&gt;&lt;td&gt;PURE YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10OY3KH-TR&lt;/td&gt;&lt;td&gt;ULTRA YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10AG3KH-TR&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10BG3KH-TR&lt;/td&gt;&lt;td&gt;BLUE GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10PB1KH-TR&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;SML10CW1KH-TR&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;

Source: http://www.ledtronics.com/ds/smd-1206/dstr0094.PDF</description>
</package>
<package name="OSTAR_4_">
<description>&lt;b&gt;OSTAR® without LENS&lt;/b&gt;&lt;p&gt;
Source: http://catalog.osram-os.com/media/_en/Graphics/00035766_0.pdf</description>
</package>
<package name="OSTAR-LENS_">
<description>&lt;b&gt;OSTAR® with LENS&lt;/b&gt;&lt;p&gt;
Source: http://catalog.osram-os.com/media/_en/Graphics/00035766_0.pdf</description>
</package>
<package name="OSTAR_6-LEW3A">
<description>&lt;b&gt;OSTAR - Lighting wihtout Optics&lt;/b&gt;&lt;p&gt;
Source: http://catalog.osram-os.com/media/_en/Graphics/00035769_0.pdf</description>
</package>
<package name="SO-8">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt; SO-8 CASE 751-07&lt;p&gt;
150-mil body, package type SN&lt;br&gt;
SOurce: http://www.onsemi.com/pub/Collateral/NUD4001-D.PDF</description>
</package>
<package name="NFSG036BT">
<description>&lt;b&gt;CHIP TYPE GREEN LED&lt;/b&gt; NFSx036xT&lt;p&gt;
Source: &lt;a href="http://www.nichia.co.jp/specification/en/product/led_library/NFSG036BT-E.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="F50380">
<description>&lt;b&gt;Z-POWER LED&lt;/b&gt;&lt;p&gt;
Source: www.zpowerled.com .. F50380.pdf</description>
</package>
<package name="P-TO263-7-1">
<description>&lt;b&gt;P-TO263-7-1&lt;/b&gt; (Plastic Transistor Single Outline)&lt;p&gt;
Source: Infineon .. tle4242.pdf</description>
</package>
<package name="P-LCC-6_TOPLED">
<description>&lt;b&gt;P-LCC-6 TOPLED MULTILED®&lt;/b&gt;&lt;p&gt;
Source: OSRAM - LRTB_G6TG.pdf</description>
</package>
<package name="DUOLED-A-5MM">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/green, red/yellow), 5 mm, round, common Anode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
</package>
<package name="DUOLED-C-5MM">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/green, red/yellow), 5 mm, round, common Cathode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
</package>
<package name="LED10MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
10 mm, round</description>
</package>
<package name="LED_BLINK">
<description>&lt;B&gt;LED BLINK&lt;/B&gt;
Symbol for Silkscreen layer</description>
</package>
<package name="LED_OFF">
<description>&lt;B&gt;LED OFF&lt;/B&gt;
Symbol for Silkscreen layer</description>
</package>
<package name="LED_ON">
<description>&lt;B&gt;LED ON&lt;/B&gt;
Symbol for Silkscreen layer</description>
</package>
<package name="ACULED-RGB">
<description>&lt;b&gt;ACULED&lt;/b&gt;&lt;p&gt;
Source: http://optoelectronics.perkinelmer.com/content/Datasheets/DTS_ACULED.pdf</description>
</package>
<package name="ACULEDVHL">
<description>&lt;b&gt;ACULED® VHL&lt;/b&gt; Standard Monochromatic and Multi-Colored Four-Chip LED&lt;p&gt;
Source: http://optoelectronics.perkinelmer.com/content/Datasheets/DTS_ACULEDVHL.pdf</description>
</package>
<package name="LUXEON_REBEL">
<description>&lt;b&gt;LUXEON® Rebel LED&lt;/b&gt;&lt;p&gt;

Set DRC - Clearance - &lt;b&gt;Same Signals&lt;/b&gt; to &lt;b&gt;0&lt;/b&gt; to avoid DRC error message for Pad in SMD.&lt;br&gt;
Please read the Device's Description how to connect it correctly in the Schematic.&lt;p&gt;
Source: http://www.lumileds.com/pdfs/AB32.pdf</description>
</package>
<package name="LUXEON_REBEL-REFERENCE">
<description>Generated from &lt;b&gt;Luxeon Rebel Footprint _customer.dxf&lt;/b&gt;&lt;p&gt;
from &amp;lt;rudi.hechfellner@philips.com&amp;gt;</description>
</package>
<package name="LRTB_G6SG">
<description>&lt;b&gt;LRTB G6SG&lt;/b&gt; 6-lead TOPLED®&lt;p&gt;
Source: OSRAM Opto Semiconductors ... LRTB_G6SG_Pb_free.pdf</description>
</package>
<package name="OVSTRGBBCR8">
<description>&lt;b&gt;Full Color PLCC6 LED&lt;/b&gt; OVSTRGBBCR8&lt;p&gt;
Source: www.optekinc.com  .. ovstrgbbcr8.pdf</description>
</package>
<package name="LP2C63-ST-RGB-SR0">
<description>&lt;b&gt;1.5W RGB HIGH POWER LED&lt;/b&gt;&lt;p&gt;
LEDTECH ELECTRONICS CORP.&lt;br&gt;
Source: LP2C63-ST-RGB-SR0.SPEC.pdf</description>
</package>
<package name="W57B">
<description>&lt;b&gt;Golden Dragon® 1 Watt LED&lt;/b&gt;&lt;p&gt;
Source: OSRAM la_ly_w57b.pdf</description>
</package>
<package name="W5KM">
<description>&lt;b&gt;Golden DRAGON® ARGUS® LED&lt;/b&gt;&lt;p&gt;
Place TH-Gate and connect pins in schematic.&lt;br&gt;
Set DRC-Clearance - Same Signals to 0mm in board.&lt;br&gt;
Source: catalog.osram-os.com .. LD_LB_LT_W5KM_Pb_free.pdf</description>
</package>
<package name="PLCC2">
<description>&lt;b&gt;LC TOPLED®, Low Current LED,&lt;/b&gt;&lt;p&gt;
LS T679, LY T679, LG T679&lt;br&gt;
Source: http://catalog.osram-os.com .. LG_LS_LY_T679_OBS.pdf</description>
</package>
<package name="KA-3528ASYC">
<description>&lt;b&gt;SURFACE MOUNT LED LAMP&lt;/b&gt; 3.5x2.8mm&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/KA-3528ASYC(Ver1189474662.1)</description>
</package>
<package name="W51">
<description>&lt;b&gt;Golden DRAGON® with Lens&lt;/b&gt; Enhanced Thinfilm LED&lt;p&gt;
Source: LA_LR_LY_W51M_Pb_free[1].pdf</description>
</package>
<package name="W51-COOL">
<description>&lt;b&gt;Golden DRAGON® with Lens&lt;/b&gt; Enhanced Thinfilm LED&lt;p&gt;
with thermal holes&lt;br&gt;
Source: LA_LR_LY_W51M_Pb_free[1].pdf</description>
</package>
<package name="GM1BW78140A">
<description>&lt;b&gt;High Brightness Chip LED (White)&lt;/b&gt;&lt;p&gt;
Source: http://document.sharpsma.com/files/GM1BW78140A.pdf</description>
</package>
<package name="GM1WA55311A">
<description>&lt;b&gt;Chip LED RGB&lt;/b&gt;&lt;p&gt;
Source: http://document.sharpsma.com/files/GM1WA55311A_SS.pdf</description>
</package>
<package name="GM5WA94310A">
<description>&lt;b&gt;Chip LED&lt;/b&gt; RGB&lt;p&gt;
Source: http://document.sharpsma.com/files/GM5WA94310A_SS.pdf</description>
</package>
<package name="GM5BW96385A">
<description>&lt;b&gt;High brightness White Color LED&lt;/b&gt;&lt;p&gt;
Source: http://document.sharpsma.com/files/GM5BW96385A.pdf</description>
</package>
<package name="NSSM038A">
<description>&lt;b&gt;3 LED (RGB) package&lt;/b&gt;&lt;p&gt;
&lt;i&gt;&lt;b&gt;Set DRC Clearance - Same Signals - Smd | Smd,  0mm&lt;/b&gt;&lt;/i&gt;&lt;p&gt;
Source: NICIA CORPORATION .. NSSM038AT-E.PDF</description>
</package>
<package name="W724C0">
<description>&lt;b&gt;Z-Power LED&lt;/b&gt;&lt;p&gt;
Source: http://www.acriche.com .. W724C0.pdf</description>
</package>
<package name="F50360">
<description>&lt;b&gt;Full color Z-Power LED RGB&lt;/b&gt;&lt;p&gt;
Source: http://www.seoulsemicon.co.kr .. F50360.pdf</description>
</package>
<package name="Z-POWER-LED-DOME-TYPE">
<description>&lt;b&gt;Z-Power LED&lt;/b&gt;&lt;p&gt;
Source: http://www.seoulsemicon.co.kr .. X42180.pdf</description>
</package>
<package name="Z-POWER-LED-PCB-TYPE">
<description>&lt;b&gt;Z-Power LED&lt;/b&gt;&lt;p&gt;
Source: http://www.seoulsemicon.co.kr .. X42182.pdf</description>
</package>
<package name="LZC-00CW40">
<description>&lt;b&gt;High Luminous Efficacy LED Emitter&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ledengin.com/products/40wLZ/LZC-00CW40.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="LZ1-00WW03">
<description>&lt;b&gt;High Luminous Efficacy LED Emitter&lt;/b&gt;&lt;p&gt;
Source: http://www.ledengin.com/products/3wLZ/LZ1-00WW03.pdf</description>
</package>
<package name="LZ4-00WW10">
<description>&lt;b&gt;High Luminous Efficacy 10W LED&lt;/b&gt;&lt;p&gt;
Source: http://www.ledengin.com/products/10wLZ/LZ4-00WW10.pdf</description>
</package>
<package name="CREE_XLAMP">
<description>&lt;b&gt;Cree® XLamp® XP-E LEDs&lt;/b&gt;&lt;p&gt;
Source: www.cree.com/xlamp .. XLampXP-E.pdf</description>
</package>
<package name="DUOLED-A-3MM">
<description>&lt;b&gt;T-1(3mm) BI-COLOR INDICATOR LAMP&lt;/b&gt;&lt;p&gt;
Source: Kingbright .. 2_colour_led_.pdf</description>
</package>
<package name="TLUV5300">
<description>&lt;b&gt;Bicolor LED 5 mm&lt;/b&gt; Untinted Diffused Package&lt;p&gt;
Source: www.vishay.com .. Bi-Color LED Vashay TLUV5300.pdf</description>
</package>
<package name="P47F-TOP">
<description>&lt;b&gt;PointLED® Enhanced Thinfilm LED&lt;/b&gt; TOP mount&lt;p&gt;
Source: http://catalog.osram-os.com .. LA_LR_LS_LY_P47F_Pb_free.pdf</description>
</package>
<package name="P47F-BOTTOM">
<description>&lt;b&gt;PointLED® Enhanced Thinfilm LED&lt;/b&gt; BOTTOM mount&lt;p&gt;
Source: http://catalog.osram-os.com .. LA_LR_LS_LY_P47F_Pb_free.pdf</description>
</package>
<package name="L-59EGW-CA">
<description>&lt;b&gt;T-1 4/4 (5mm) BI-POLAR AND BI-COLOR INDICATOR LAMPS&lt;/b&gt;&lt;p&gt;
Source: Kingbright L-59 Series</description>
</package>
<package name="CP41B">
<description>&lt;b&gt;Cree® P4 LED CP41B-WES/WGS&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/LEDlamps/CP41B-WES&amp;WGS.pdf"&gt; Data sheet&lt;/a&gt;</description>
</package>
<package name="CLN6A">
<description>&lt;b&gt;Cree® CLN6A-WKW/MKW&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/LEDlamps/CLN6A%28979%29.pdf"&gt; Data sheet&lt;/a&gt;</description>
</package>
<package name="PB3XX301V050A">
<description>&lt;b&gt;RGB LED&lt;/b&gt; with integrated controller chip&lt;p&gt;
Source: &lt;a href="http://www.kirronlightcomponents.com/produkte/dyco-led1/"&gt; Data sheedt &lt;/a&gt; DycoLED.pdf&lt;br&gt;
http://www.ubleds.com.tw</description>
</package>
<package name="MX6">
<description>&lt;b&gt;Cree® XLamp® MX-6 LEDs&lt;/b&gt; with cooling drills for FR4&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/XLampMX-6.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="MX6-ALU">
<description>&lt;b&gt;Cree® XLamp® MX-6 LEDs&lt;/b&gt; for mounting on ALU PCBs&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/XLampMX-6.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="SPHWHTHAD605S0W0U4">
<description>&lt;b&gt;HV-AC HIGH POWER LED&lt;/b&gt;&lt;p&gt;
Source: SAMSUNG SPHWHTHAD605S0W0U4.pdf</description>
</package>
<package name="ML-E">
<description>&lt;b&gt;Cree® XLamp® ML-E LEDs&lt;/b&gt; 1/2 watt, 3.5 x 3.5 mm&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/XLampML-E.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="CREE-XLAMP-XM-L">
<description>&lt;b&gt;Cree® XLamp® XM-L LEDs&lt;/b&gt;&lt;p&gt;
Source: http://www.cree.com</description>
</package>
<package name="P-LCC4-T676">
<description>Source: http://docs-europe.electrocomponents.com/webdocs/08c3/0900766b808c36ca.pdf</description>
</package>
<package name="P-LCC4-0">
<description>&lt;b&gt;white P-LCC-4 package&lt;/b&gt;&lt;p&gt;
Source: http://docs-europe.electrocomponents.com/webdocs/08c3/0900766b808c36ca.pdf</description>
</package>
<package name="LED3MM_H">
<description>&lt;b&gt;3mm LED, horizontal&lt;/b&gt; PADs in line&lt;p&gt;</description>
</package>
<package name="LED3MM_H7,5MM">
<description>&lt;b&gt;LED 3mm horizontal&lt;/b&gt; ( 7,5mm from pad to abut)&lt;p&gt;
Source: Kingbright, qgL-7104LYD_data_e.pdf</description>
</package>
<package name="LED5MM_H6,0MM">
<description>&lt;b&gt;LED 5mm horizontal&lt;/b&gt; ( 6mm from pad to abut)&lt;p&gt;
Source: LUCKY LIGHT,  dkSetron_LED-w_EN.pdf</description>
</package>
<package name="LZ4-40U600">
<description>&lt;b&gt;High Efficacy 365nm UV LED Emitter&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ledengin.com/files/products/LZ4/LZ4-00U600.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="LUXEON_5630">
<description>&lt;b&gt;LUXEON 5630 Mid-Power LEDs&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="www.philipslumileds.com/uploads/351/DS201-pdf"&gt; Data sheet &lt;/a&gt;&lt;br&gt;
Lumileds 5630 Datasheet DS201 20130228 ©2013 Philips Lumileds Lighting Company.</description>
</package>
<package name="PC56H19_V0">
<description>&lt;b&gt;Lextar&lt;/b&gt; white SMD LED&lt;p&gt;
Source: PC56H19_20150317.pdf&lt;br&gt;
www.lextar.com</description>
</package>
</packages>
<symbols>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-A">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-D">
<pin name="C" direction="pas"/>
<pin name="AR" direction="pas"/>
<pin name="AG" direction="pas"/>
</symbol>
<symbol name="LED-RGB">
<pin name="CGREEN" direction="pas"/>
<pin name="CBLUE" direction="pas"/>
<pin name="CRED" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="LED-PAD">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="16-SEG-MSA5XX">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
<pin name="17" direction="pas"/>
<pin name="18" direction="pas"/>
</symbol>
<symbol name="SA08-7SEGMENT">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="AK@1" direction="pas"/>
<pin name="AK@2" direction="pas"/>
<pin name="AK@3" direction="pas"/>
<pin name="AK@4" direction="pas"/>
</symbol>
<symbol name="5-SEGMENT">
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="H" direction="pas"/>
<pin name="J" direction="pas"/>
<pin name="DP2" direction="pas"/>
<pin name="B'" direction="pas"/>
<pin name="C'" direction="pas"/>
<pin name="G'" direction="pas"/>
<pin name="H'" direction="pas"/>
<pin name="J'" direction="pas"/>
<pin name="DP2'" direction="pas"/>
<pin name="B_" direction="pas"/>
</symbol>
<symbol name="SA08-21">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="AN@1" direction="pas"/>
<pin name="AN@2" direction="pas"/>
<pin name="AN@3" direction="pas"/>
<pin name="D@1" direction="pas"/>
<pin name="E@1" direction="pas"/>
</symbol>
<symbol name="SC08-21">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="K@1" direction="pas"/>
<pin name="K@2" direction="pas"/>
<pin name="K@3" direction="pas"/>
<pin name="K@4" direction="pas"/>
<pin name="E@1" direction="pas"/>
</symbol>
<symbol name="LED-A2C2">
<pin name="C@1" direction="pas"/>
<pin name="A@1" direction="pas"/>
<pin name="A@2" direction="pas"/>
<pin name="C@2" direction="pas"/>
</symbol>
<symbol name="OSTAR4">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="OSTAR6">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="NUD4001">
<pin name="VIN" direction="in"/>
<pin name="REXT" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="IOUT" direction="pas"/>
<pin name="BOOST" direction="pas"/>
</symbol>
<symbol name="NUD4011">
<pin name="VIN" direction="in"/>
<pin name="REXT" direction="pas"/>
<pin name="PWM" direction="pas"/>
<pin name="IOUT" direction="pas"/>
<pin name="BOOST" direction="pas"/>
</symbol>
<symbol name="F50380">
<pin name="B-" direction="pas"/>
<pin name="B+" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="R-" direction="pas"/>
<pin name="R+" direction="pas"/>
</symbol>
<symbol name="THERMAL">
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="TLE4242">
<pin name="IN" direction="in"/>
<pin name="PWM" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="D" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="ST" direction="oc"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DUOLED-RG-A">
<pin name="A" direction="pas"/>
<pin name="CR" direction="pas"/>
<pin name="CG" direction="pas"/>
</symbol>
<symbol name="DUOLED-RG-C">
<pin name="C" direction="pas"/>
<pin name="AR" direction="pas"/>
<pin name="AG" direction="pas"/>
</symbol>
<symbol name="DUOLED-RY-A">
<pin name="A" direction="pas"/>
<pin name="CR" direction="pas"/>
<pin name="CY" direction="pas"/>
</symbol>
<symbol name="DUOLED-RY-C">
<pin name="C" direction="pas"/>
<pin name="AR" direction="pas"/>
<pin name="AY" direction="pas"/>
</symbol>
<symbol name="ACULED-RGB">
<pin name="RC" direction="pas"/>
<pin name="BC" direction="pas"/>
<pin name="GC" direction="pas"/>
<pin name="GA" direction="pas"/>
<pin name="BA" direction="pas"/>
<pin name="RA" direction="pas"/>
</symbol>
<symbol name="LED+D">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED4P">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-4">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-RGB-A">
<pin name="CGREEN" direction="pas"/>
<pin name="CBLUE" direction="pas"/>
<pin name="CRED" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="NSSM038A-RGB">
<pin name="BC" direction="pas"/>
<pin name="BA" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="RA" direction="pas"/>
<pin name="GC" direction="pas"/>
<pin name="GA" direction="pas"/>
</symbol>
<symbol name="LED4-A2C2">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="LED-RGB-D">
<pin name="BC" direction="pas"/>
<pin name="GC" direction="pas"/>
<pin name="RC" direction="pas"/>
<pin name="RA" direction="pas"/>
<pin name="GA" direction="pas"/>
<pin name="BA" direction="pas"/>
</symbol>
<symbol name="LED-2X6">
<pin name="A1" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="A2" direction="pas"/>
</symbol>
<symbol name="DUOLED-OG-C">
<pin name="CC" direction="pas"/>
<pin name="AO" direction="pas"/>
<pin name="AG" direction="pas"/>
</symbol>
<symbol name="PB3XX301V050A">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="DI" direction="in"/>
<pin name="CI" direction="in"/>
<pin name="DO" direction="out"/>
<pin name="CO" direction="out"/>
</symbol>
<symbol name="SPHWHTHAD605S0W0U4">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LB10" prefix="DZ">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
10-LED bar graph, DIL, Siemens</description>
<gates>
<gate name="-1" symbol="LED-A"/>
<gate name="-2" symbol="LED-A"/>
<gate name="-3" symbol="LED-A"/>
<gate name="-4" symbol="LED-A"/>
<gate name="-5" symbol="LED-A"/>
<gate name="-6" symbol="LED-A"/>
<gate name="-7" symbol="LED-A"/>
<gate name="-8" symbol="LED-A"/>
<gate name="-9" symbol="LED-A"/>
<gate name="-10" symbol="LED-A"/>
</gates>
<devices>
<device name="" package="LB10">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="C" pad="20"/>
<connect gate="-10" pin="A" pad="10"/>
<connect gate="-10" pin="C" pad="11"/>
<connect gate="-2" pin="A" pad="2"/>
<connect gate="-2" pin="C" pad="19"/>
<connect gate="-3" pin="A" pad="3"/>
<connect gate="-3" pin="C" pad="18"/>
<connect gate="-4" pin="A" pad="4"/>
<connect gate="-4" pin="C" pad="17"/>
<connect gate="-5" pin="A" pad="5"/>
<connect gate="-5" pin="C" pad="16"/>
<connect gate="-6" pin="A" pad="6"/>
<connect gate="-6" pin="C" pad="15"/>
<connect gate="-7" pin="A" pad="7"/>
<connect gate="-7" pin="C" pad="14"/>
<connect gate="-8" pin="A" pad="8"/>
<connect gate="-8" pin="C" pad="13"/>
<connect gate="-9" pin="A" pad="9"/>
<connect gate="-9" pin="C" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U57X32" prefix="D">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
rectangle, 5.7 x 3.2 mm</description>
<gates>
<gate name="1" symbol="LED"/>
</gates>
<devices>
<device name="" package="U57X32">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUOLED2X5" prefix="D" uservalue="yes">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;p&gt;
2 colors, 2.5 x 5 mm, recangle</description>
<gates>
<gate name="1" symbol="LED-D"/>
</gates>
<devices>
<device name="" package="DUOLED2X5">
<connects>
<connect gate="1" pin="AG" pad="AG"/>
<connect gate="1" pin="AR" pad="AR"/>
<connect gate="1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUOLED5MM" prefix="D" uservalue="yes">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;p&gt;
2 colors, 5 mm, round</description>
<gates>
<gate name="1" symbol="LED-D"/>
</gates>
<devices>
<device name="" package="DUOLED5MM">
<connects>
<connect gate="1" pin="AG" pad="AG"/>
<connect gate="1" pin="AR" pad="AR"/>
<connect gate="1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZR182" prefix="DZ">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
2 LEDs, Siemens</description>
<gates>
<gate name="-1" symbol="LED"/>
<gate name="-2" symbol="LED"/>
</gates>
<devices>
<device name="" package="LZR182">
<connects>
<connect gate="-1" pin="A" pad="A1"/>
<connect gate="-1" pin="C" pad="K1"/>
<connect gate="-2" pin="A" pad="A2"/>
<connect gate="-2" pin="C" pad="K2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZR183" prefix="DZ">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
3 LEDs, Siemens</description>
<gates>
<gate name="-1" symbol="LED"/>
<gate name="-2" symbol="LED"/>
<gate name="-3" symbol="LED"/>
</gates>
<devices>
<device name="" package="LZR183">
<connects>
<connect gate="-1" pin="A" pad="A1"/>
<connect gate="-1" pin="C" pad="K1"/>
<connect gate="-2" pin="A" pad="A2"/>
<connect gate="-2" pin="C" pad="K2"/>
<connect gate="-3" pin="A" pad="A3"/>
<connect gate="-3" pin="C" pad="K3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZR184" prefix="DZ">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
4 LEDs, Siemens</description>
<gates>
<gate name="-1" symbol="LED"/>
<gate name="-2" symbol="LED"/>
<gate name="-3" symbol="LED"/>
<gate name="-4" symbol="LED"/>
</gates>
<devices>
<device name="" package="LZR184">
<connects>
<connect gate="-1" pin="A" pad="A1"/>
<connect gate="-1" pin="C" pad="K1"/>
<connect gate="-2" pin="A" pad="A2"/>
<connect gate="-2" pin="C" pad="K2"/>
<connect gate="-3" pin="A" pad="A3"/>
<connect gate="-3" pin="C" pad="K3"/>
<connect gate="-4" pin="A" pad="A4"/>
<connect gate="-4" pin="C" pad="K4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZR185" prefix="DZ">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
5 LEDs, Siemens</description>
<gates>
<gate name="-1" symbol="LED"/>
<gate name="-2" symbol="LED"/>
<gate name="-3" symbol="LED"/>
<gate name="-4" symbol="LED"/>
<gate name="-5" symbol="LED"/>
</gates>
<devices>
<device name="" package="LZR185">
<connects>
<connect gate="-1" pin="A" pad="A1"/>
<connect gate="-1" pin="C" pad="K1"/>
<connect gate="-2" pin="A" pad="A2"/>
<connect gate="-2" pin="C" pad="K2"/>
<connect gate="-3" pin="A" pad="A3"/>
<connect gate="-3" pin="C" pad="K3"/>
<connect gate="-4" pin="A" pad="A4"/>
<connect gate="-4" pin="C" pad="K4"/>
<connect gate="-5" pin="A" pad="A5"/>
<connect gate="-5" pin="C" pad="K5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD266" prefix="DZ">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
6 LEDs, Siemens</description>
<gates>
<gate name="-1" symbol="LED"/>
<gate name="-2" symbol="LED"/>
<gate name="-3" symbol="LED"/>
<gate name="-4" symbol="LED"/>
<gate name="-5" symbol="LED"/>
<gate name="-6" symbol="LED"/>
</gates>
<devices>
<device name="" package="LD266">
<connects>
<connect gate="-1" pin="A" pad="A1"/>
<connect gate="-1" pin="C" pad="K1"/>
<connect gate="-2" pin="A" pad="A2"/>
<connect gate="-2" pin="C" pad="K2"/>
<connect gate="-3" pin="A" pad="A3"/>
<connect gate="-3" pin="C" pad="K3"/>
<connect gate="-4" pin="A" pad="A4"/>
<connect gate="-4" pin="C" pad="K4"/>
<connect gate="-5" pin="A" pad="A5"/>
<connect gate="-5" pin="C" pad="K5"/>
<connect gate="-6" pin="A" pad="A6"/>
<connect gate="-6" pin="C" pad="K6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD269" prefix="DZ">
<description>&lt;B&gt;LED BLOCK&lt;/B&gt;&lt;p&gt;
9 LEDs, Siemens</description>
<gates>
<gate name="-1" symbol="LED"/>
<gate name="-2" symbol="LED"/>
<gate name="-3" symbol="LED"/>
<gate name="-4" symbol="LED"/>
<gate name="-5" symbol="LED"/>
<gate name="-6" symbol="LED"/>
<gate name="-7" symbol="LED"/>
<gate name="-8" symbol="LED"/>
<gate name="-9" symbol="LED"/>
</gates>
<devices>
<device name="" package="LD269">
<connects>
<connect gate="-1" pin="A" pad="A1"/>
<connect gate="-1" pin="C" pad="K1"/>
<connect gate="-2" pin="A" pad="A2"/>
<connect gate="-2" pin="C" pad="K2"/>
<connect gate="-3" pin="A" pad="A3"/>
<connect gate="-3" pin="C" pad="K3"/>
<connect gate="-4" pin="A" pad="A4"/>
<connect gate="-4" pin="C" pad="K4"/>
<connect gate="-5" pin="A" pad="A5"/>
<connect gate="-5" pin="C" pad="K5"/>
<connect gate="-6" pin="A" pad="A6"/>
<connect gate="-6" pin="C" pad="K6"/>
<connect gate="-7" pin="A" pad="A7"/>
<connect gate="-7" pin="C" pad="K7"/>
<connect gate="-8" pin="A" pad="A8"/>
<connect gate="-8" pin="C" pad="K8"/>
<connect gate="-9" pin="A" pad="A9"/>
<connect gate="-9" pin="C" pad="K9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SFH482" prefix="D">
<description>&lt;B&gt;IR LED&lt;/B&gt;&lt;p&gt;
infrared emitting diode, Infineon</description>
<gates>
<gate name="1" symbol="LED"/>
</gates>
<devices>
<device name="" package="SFH482">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LED&lt;/b&gt;&lt;p&gt;
&lt;u&gt;OSRAM&lt;/u&gt;:&lt;br&gt;

- &lt;u&gt;CHIPLED&lt;/u&gt;&lt;br&gt;
LG R971, LG N971, LY N971, LG Q971, LY Q971, LO R971, LY R971
LH N974, LH R974&lt;br&gt;
LS Q976, LO Q976, LY Q976&lt;br&gt;
LO Q996&lt;br&gt;

- &lt;u&gt;Hyper CHIPLED&lt;/u&gt;&lt;br&gt;
LW Q18S&lt;br&gt;
LB Q993, LB Q99A, LB R99A&lt;br&gt;

- &lt;u&gt;SideLED&lt;/u&gt;&lt;br&gt;
LS A670, LO A670, LY A670, LG A670, LP A670&lt;br&gt;
LB A673, LV A673, LT A673, LW A673&lt;br&gt;
LH A674&lt;br&gt;
LY A675&lt;br&gt;
LS A676, LA A676, LO A676, LY A676, LW A676&lt;br&gt;
LS A679, LY A679, LG A679&lt;br&gt;

-  &lt;u&gt;Hyper Micro SIDELED®&lt;/u&gt;&lt;br&gt;
LS Y876, LA Y876, LO Y876, LY Y876&lt;br&gt;
LT Y87S&lt;br&gt;

- &lt;u&gt;SmartLED&lt;/u&gt;&lt;br&gt;
LW L88C, LW L88S&lt;br&gt;
LB L89C, LB L89S, LG L890&lt;br&gt;
LS L89K, LO L89K, LY L89K&lt;br&gt;
LS L896, LA L896, LO L896, LY L896&lt;br&gt;

- &lt;u&gt;TOPLED&lt;/u&gt;&lt;br&gt;
LS T670, LO T670, LY T670, LG T670, LP T670&lt;br&gt;
LSG T670, LSP T670, LSY T670, LOP T670, LYG T670&lt;br&gt;
LG T671, LOG T671, LSG T671&lt;br&gt;
LB T673, LV T673, LT T673, LW T673&lt;br&gt;
LH T674&lt;br&gt;
LS T676, LA T676, LO T676, LY T676, LB T676, LH T676, LSB T676, LW T676&lt;br&gt;
LB T67C, LV T67C, LT T67C, LS T67K, LO T67K, LY T67K, LW E67C&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B, LB E67C, LV E67C, LT E67C&lt;br&gt;
LW T67C&lt;br&gt;
LS T679, LY T679, LG T679&lt;br&gt;
LS T770, LO T770, LY T770, LG T770, LP T770&lt;br&gt;
LB T773, LV T773, LT T773, LW T773&lt;br&gt;
LH T774&lt;br&gt;
LS E675, LA E675, LY E675, LS T675&lt;br&gt;
LS T776, LA T776, LO T776, LY T776, LB T776&lt;br&gt;
LHGB T686&lt;br&gt;
LT T68C, LB T68C&lt;br&gt;

- &lt;u&gt;Hyper Mini TOPLED®&lt;/u&gt;&lt;br&gt;
LB M676&lt;br&gt;

- &lt;u&gt;Mini TOPLED Santana®&lt;/u&gt;&lt;br&gt;
LG M470&lt;br&gt;
LS M47K, LO M47K, LY M47K
&lt;p&gt;
Source: http://www.osram.convergy.de&lt;p&gt;

&lt;u&gt;LUXEON:&lt;/u&gt;&lt;br&gt;
- &lt;u&gt;LUMILED®&lt;/u&gt;&lt;br&gt;
LXK2-PW12-R00, LXK2-PW12-S00, LXK2-PW14-U00, LXK2-PW14-V00&lt;br&gt;
LXK2-PM12-R00, LXK2-PM12-S00, LXK2-PM14-U00&lt;br&gt;
LXK2-PE12-Q00, LXK2-PE12-R00, LXK2-PE12-S00, LXK2-PE14-T00, LXK2-PE14-U00&lt;br&gt;
LXK2-PB12-K00, LXK2-PB12-L00, LXK2-PB12-M00, LXK2-PB14-N00, LXK2-PB14-P00, LXK2-PB14-Q00&lt;br&gt;
LXK2-PR12-L00, LXK2-PR12-M00, LXK2-PR14-Q00, LXK2-PR14-R00&lt;br&gt;
LXK2-PD12-Q00, LXK2-PD12-R00, LXK2-PD12-S00&lt;br&gt;
LXK2-PH12-R00, LXK2-PH12-S00&lt;br&gt;
LXK2-PL12-P00, LXK2-PL12-Q00, LXK2-PL12-R00
&lt;p&gt;
Source: www.luxeon.com&lt;p&gt;

&lt;u&gt;KINGBRIGHT:&lt;/U&gt;&lt;p&gt;
KA-3528ASYC&lt;br&gt;
Source: www.kingbright.com</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="SMT1206" package="1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LD260" package="LD260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR2X5" package="LED2X5">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3MM" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5MM" package="LED5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LSU260" package="LSU260">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LZR181" package="LZR181">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B152" package="Q62902-B152">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B153" package="Q62902-B153">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B155" package="Q62902-B155">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B156" package="Q62902-B156">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH480" package="SFH480">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SFH482" package="SFH482">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SQR5.7X3.2" package="U57X32">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IRL80A" package="IRL80A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2" package="P-LCC-2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MINI-TOP" package="OSRAM-MINI-TOP-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SIDELED" package="OSRAM-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMART-LED" package="SMART-LED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="B"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-2-BACK" package="P-LCC-2-TOPLED-RG">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MICRO-SIDELED" package="MICRO-SIDELED">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-4" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0603" package="CHIP-LED0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIP-LED0805" package="CHIP-LED0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TOPLED-SANTANA" package="MINI-TOPLED-SANTANA">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0805" package="CHIPLED_0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_1206" package="CHIPLED_1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED_0603" package="CHIPLED_0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CHIPLED-0603-TTW" package="CHIPLED-0603-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="SMARTLED-TTW">
<connects>
<connect gate="G$1" pin="A" pad="A@1"/>
<connect gate="G$1" pin="C" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED+" package="LUMILED+">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LUMILED" package="LUMILED">
<connects>
<connect gate="G$1" pin="A" pad="2+"/>
<connect gate="G$1" pin="C" pad="4-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="10MM" package="LED10MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KA-3528ASYC" package="KA-3528ASYC">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML0805" package="SML0805">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML1206" package="SML1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SML0603" package="SML0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOPLED-3" prefix="LED" uservalue="yes">
<description>&lt;b&gt;OSRAM&lt;/b&gt;&lt;p&gt;
- &lt;u&gt;Hyper Multi TOPLED® (RGB)&lt;/u&gt;&lt;br&gt;
LB E673, LV E673, LT E673&lt;br&gt;
- &lt;u&gt;Power TOPLED® Enhanced optical Power LED (HOP2000)&lt;/u&gt;&lt;br&gt;
LS E67B, LA E67B, LO E67B, LY E67B&lt;br&gt;
- &lt;u&gt;Hyper Multi TOPLED® Enhanced optical Power LED (HOP2000 / ATON®)&lt;/u&gt;&lt;br&gt;
LATB T66B&lt;br&gt;
- &lt;u&gt;Hyper Multi TOPLED® Hyper-Bright LED&lt;/u&gt;&lt;br&gt;
LATB T686&lt;br&gt;

&lt;p&gt;
Source: http://www.osram.convergy.de/</description>
<gates>
<gate name="G$1" symbol="LED-RGB"/>
</gates>
<devices>
<device name="P-LCC-4" package="P-LCC-4">
<connects>
<connect gate="G$1" pin="A2" pad="A"/>
<connect gate="G$1" pin="CBLUE" pad="C@3"/>
<connect gate="G$1" pin="CGREEN" pad="C@4"/>
<connect gate="G$1" pin="CRED" pad="C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="P-LCC-4-3">
<connects>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="CBLUE" pad="3"/>
<connect gate="G$1" pin="CGREEN" pad="4"/>
<connect gate="G$1" pin="CRED" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TOPLED-2-" prefix="LED" uservalue="yes">
<description>&lt;b&gt;Multi TOPLED® (two color)&lt;/b&gt;&lt;p&gt;
LG T672, LP T672&lt;br&gt;
LSY T67B&lt;br&gt;
LSW T67C&lt;br&gt;
LSY T675&lt;br&gt;
LSY T676&lt;br&gt;
LSG T677&lt;br&gt;
LSG T770&lt;br&gt;

Source: http://www.osram.convergy.de/</description>
<gates>
<gate name="A" symbol="LED-PAD"/>
<gate name="B" symbol="LED-PAD"/>
</gates>
<devices>
<device name="/" package="P-LCC-4/2">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="B" pin="A" pad="4"/>
<connect gate="B" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-" package="P-LCC-4-2">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="C" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P-LCC-4-RG" package="PLCC4-TOPLED-RG">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="B" pin="A" pad="4"/>
<connect gate="B" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSA5*C" prefix="LED">
<description>&lt;b&gt;16 Segment, Single Digit Alpha-Numeric Display&lt;/b&gt; 0.5 Inch (12.7 mm)&lt;p&gt;
Source: www.fairchildsemi.com/ds/MS/MSA5480C.pdf</description>
<gates>
<gate name="G$1" symbol="16-SEG-MSA5XX"/>
</gates>
<devices>
<device name="" package="MSA5XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="17" pad="17"/>
<connect gate="G$1" pin="18" pad="18"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="160"/>
<technology name="180"/>
<technology name="360"/>
<technology name="380"/>
<technology name="460"/>
<technology name="480"/>
<technology name="960"/>
<technology name="980"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="S*08" prefix="LD">
<description>&lt;b&gt;Kingbright 20mm (0.8Inch) Single Digit Numeric Display&lt;/b&gt;&lt;p&gt;
Source: SA08-11SRWA.pdf</description>
<gates>
<gate name="G$1" symbol="SA08-7SEGMENT"/>
</gates>
<devices>
<device name="-11" package="SA08">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="AK@1" pad="3"/>
<connect gate="G$1" pin="AK@2" pad="5"/>
<connect gate="G$1" pin="AK@3" pad="11"/>
<connect gate="G$1" pin="AK@4" pad="16"/>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="C" pad="12"/>
<connect gate="G$1" pin="D" pad="10"/>
<connect gate="G$1" pin="DP" pad="9"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$1" pin="F" pad="2"/>
<connect gate="G$1" pin="G" pad="13"/>
</connects>
<technologies>
<technology name="A"/>
<technology name="C"/>
</technologies>
</device>
<device name="-12" package="SA08">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="AK@1" pad="3"/>
<connect gate="G$1" pin="AK@2" pad="5"/>
<connect gate="G$1" pin="AK@3" pad="11"/>
<connect gate="G$1" pin="AK@4" pad="16"/>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="C" pad="12"/>
<connect gate="G$1" pin="D" pad="10"/>
<connect gate="G$1" pin="DP" pad="6"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$1" pin="F" pad="2"/>
<connect gate="G$1" pin="G" pad="13"/>
</connects>
<technologies>
<technology name="A"/>
<technology name="C"/>
</technologies>
</device>
<device name="-21" package="SA08-21">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="AK@1" pad="4"/>
<connect gate="G$1" pin="AK@2" pad="9"/>
<connect gate="G$1" pin="AK@3" pad="12"/>
<connect gate="G$1" pin="AK@4" pad="17"/>
<connect gate="G$1" pin="B" pad="15"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="D" pad="11"/>
<connect gate="G$1" pin="DP" pad="10"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="F" pad="3"/>
<connect gate="G$1" pin="G" pad="14"/>
</connects>
<technologies>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA08-21" prefix="LD">
<description>&lt;b&gt;Kingbright 20mm (0.8Inch) Single Digit Numeric Display&lt;/b&gt;&lt;p&gt;
Source: SA08-11SRWA.pdf</description>
<gates>
<gate name="G$1" symbol="SA08-21"/>
</gates>
<devices>
<device name="" package="SA08-21">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="AN@1" pad="4"/>
<connect gate="G$1" pin="AN@2" pad="12"/>
<connect gate="G$1" pin="AN@3" pad="17"/>
<connect gate="G$1" pin="B" pad="15"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="D" pad="11"/>
<connect gate="G$1" pin="D@1" pad="9"/>
<connect gate="G$1" pin="DP" pad="10"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="E@1" pad="7"/>
<connect gate="G$1" pin="F" pad="3"/>
<connect gate="G$1" pin="G" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FX08-11" prefix="LD">
<description>&lt;b&gt;Kingbright 20mm (0.8Inch) Single Digit Numeric Display&lt;/b&gt;&lt;p&gt;
Source: SA08-11SRWA.pdf</description>
<gates>
<gate name="G$1" symbol="5-SEGMENT"/>
</gates>
<devices>
<device name="" package="FX08">
<connects>
<connect gate="G$1" pin="B" pad="14"/>
<connect gate="G$1" pin="B'" pad="1"/>
<connect gate="G$1" pin="B_" pad="16"/>
<connect gate="G$1" pin="C" pad="12"/>
<connect gate="G$1" pin="C'" pad="11"/>
<connect gate="G$1" pin="DP2" pad="10"/>
<connect gate="G$1" pin="DP2'" pad="7"/>
<connect gate="G$1" pin="G" pad="13"/>
<connect gate="G$1" pin="G'" pad="4"/>
<connect gate="G$1" pin="H" pad="2"/>
<connect gate="G$1" pin="H'" pad="3"/>
<connect gate="G$1" pin="J" pad="6"/>
<connect gate="G$1" pin="J'" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SC08-21" prefix="LD">
<description>&lt;b&gt;Kingbright 20mm (0.8Inch) Single Digit Numeric Display&lt;/b&gt;&lt;p&gt;
Source: SA08-11SRWA.pdf</description>
<gates>
<gate name="G$1" symbol="SC08-21"/>
</gates>
<devices>
<device name="" package="SA08-21">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="B" pad="15"/>
<connect gate="G$1" pin="C" pad="13"/>
<connect gate="G$1" pin="D" pad="11"/>
<connect gate="G$1" pin="DP" pad="10"/>
<connect gate="G$1" pin="E" pad="5"/>
<connect gate="G$1" pin="E@1" pad="7"/>
<connect gate="G$1" pin="F" pad="3"/>
<connect gate="G$1" pin="G" pad="14"/>
<connect gate="G$1" pin="K@1" pad="4"/>
<connect gate="G$1" pin="K@2" pad="9"/>
<connect gate="G$1" pin="K@3" pad="12"/>
<connect gate="G$1" pin="K@4" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-2AC-" prefix="LED" uservalue="yes">
<description>&lt;b&gt;LEDs with 2 Cathode &amp; 2 Anode&lt;/b&gt;&lt;p&gt;
- Kingbright SUPER FLUX LED LAMP&lt;br&gt;
Source: www.us.kingbright.com/images/catalog/SPEC/W7676CPBC-H.pdf&lt;p&gt;
&lt;b&gt;Cree® P4 LED CP41B-WES/WGS&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/LEDlamps/CP41B-WES&amp;WGS.pdf"&gt; Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="SUPERFLUX" package="SUPERFLUX-7.6X7.6">
<connects>
<connect gate="G$1" pin="A" pad="2 4"/>
<connect gate="G$1" pin="C" pad="1 3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SMD_SUPERFLUX" package="SUPERFLUX-SMD-7.6X7.6">
<connects>
<connect gate="G$1" pin="A" pad="2 4"/>
<connect gate="G$1" pin="C" pad="1 3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP41B-WES" package="CP41B">
<connects>
<connect gate="G$1" pin="A" pad="2 3"/>
<connect gate="G$1" pin="C" pad="1 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CP41B-WGS" package="CP41B">
<connects>
<connect gate="G$1" pin="A" pad="2 3"/>
<connect gate="G$1" pin="C" pad="1 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PL006*" prefix="LD">
<description>&lt;b&gt;PLH006 Series SMD LED&lt;/b&gt; SOT23&lt;p&gt;
PLH006-WCR21 Super Red&lt;br&gt;
PLH006-WCR12 High Eff Red&lt;br&gt;
PLH006-WCG13 Green&lt;br&gt;
PLH006-WCY01 Yellow&lt;br&gt;
www.p-tec.net&lt;p&gt;
Source: http://www.wittig-electronic.de/PTEC/PL006Series.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name="-WCR12"/>
<technology name="-WCR13"/>
<technology name="-WCY01"/>
</technologies>
</device>
<device name="-WCR21" package="SOT23">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSTAR_4-" prefix="LED">
<description>&lt;b&gt;OSTAR - Lighting with / without Optics&lt;/b&gt;&lt;p&gt;
Source: http://catalog.osram-os.com/media/_en/Graphics/00035766_0.pdf</description>
<gates>
<gate name="G$1" symbol="OSTAR4"/>
</gates>
<devices>
<device name="LEWE2B-LYNL-6K8L" package="OSTAR_4_">
<connects>
<connect gate="G$1" pin="A" pad="+"/>
<connect gate="G$1" pin="C" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LEWE2B-MXPX-6K8L" package="OSTAR-LENS_">
<connects>
<connect gate="G$1" pin="A" pad="+"/>
<connect gate="G$1" pin="C" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSTAR_6-" prefix="LED">
<description>&lt;b&gt;OSTAR - Lighting wihtout Optics&lt;/b&gt;&lt;p&gt;
Source: http://catalog.osram-os.com/media/_en/Graphics/00035769_0.pdf</description>
<gates>
<gate name="G$1" symbol="OSTAR6"/>
</gates>
<devices>
<device name="LEW3A" package="OSTAR_6-LEW3A">
<connects>
<connect gate="G$1" pin="A" pad="+"/>
<connect gate="G$1" pin="C" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="LEW3B" package="OSTAR-LENS_">
<connects>
<connect gate="G$1" pin="A" pad="+"/>
<connect gate="G$1" pin="C" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD4001" prefix="IC">
<description>&lt;b&gt;High Current LED Driver&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.onsemi.com/pub/Collateral/NUD4001-D.PDF"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="B" symbol="NUD4001"/>
</gates>
<devices>
<device name="" package="SO-8">
<connects>
<connect gate="B" pin="BOOST" pad="2"/>
<connect gate="B" pin="GND" pad="4"/>
<connect gate="B" pin="IOUT" pad="5 6 7 8"/>
<connect gate="B" pin="REXT" pad="3"/>
<connect gate="B" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUD4011" prefix="IC">
<description>&lt;b&gt;Low Current LED Driver&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.onsemi.com/pub/Collateral/NUD4011-D.PDF"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="B" symbol="NUD4011"/>
</gates>
<devices>
<device name="" package="SO-8">
<connects>
<connect gate="B" pin="BOOST" pad="2"/>
<connect gate="B" pin="IOUT" pad="5 6 7 8"/>
<connect gate="B" pin="PWM" pad="4"/>
<connect gate="B" pin="REXT" pad="3"/>
<connect gate="B" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NFSG036BT" prefix="LED">
<description>&lt;b&gt;CHIP TYPE GREEN LED&lt;/b&gt; NFSx036xT&lt;p&gt;
Source: NICHIA CORPORATION .. NFSG036BT-E.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="NFSG036BT">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="F50380" prefix="LED">
<description>&lt;b&gt;Z-POWER LED&lt;/b&gt;&lt;p&gt;
Source: www.zpowerled.com .. F50380.pdf</description>
<gates>
<gate name="P" symbol="F50380"/>
<gate name="T" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="F50380">
<connects>
<connect gate="P" pin="B+" pad="B+"/>
<connect gate="P" pin="B-" pad="B-"/>
<connect gate="P" pin="G+" pad="G+"/>
<connect gate="P" pin="G-" pad="G-"/>
<connect gate="P" pin="R+" pad="R+"/>
<connect gate="P" pin="R-" pad="R-"/>
<connect gate="T" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLE4242" prefix="IC">
<description>&lt;b&gt;Adjustable LED Driver&lt;/b&gt;&lt;p&gt;
Source: Infineon .. tle4242.pdf</description>
<gates>
<gate name="P" symbol="TLE4242"/>
<gate name="T" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="P-TO263-7-1">
<connects>
<connect gate="P" pin="D" pad="6"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="IN" pad="1"/>
<connect gate="P" pin="PWM" pad="2"/>
<connect gate="P" pin="Q" pad="7"/>
<connect gate="P" pin="REF" pad="5"/>
<connect gate="P" pin="ST" pad="3"/>
<connect gate="T" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MULTILED_LRTB_G6TG" prefix="LED">
<description>&lt;b&gt;6-lead MULTILED® Enhanced optical Power LED (ThinFilm® / ThinGaN®)&lt;/b&gt;&lt;p&gt;
Source. OSRAM - LRTB_G6TG.pdf</description>
<gates>
<gate name="R" symbol="LED"/>
<gate name="G" symbol="LED"/>
<gate name="B" symbol="LED"/>
</gates>
<devices>
<device name="" package="P-LCC-6_TOPLED">
<connects>
<connect gate="B" pin="A" pad="A3"/>
<connect gate="B" pin="C" pad="C3"/>
<connect gate="G" pin="A" pad="A2"/>
<connect gate="G" pin="C" pad="C2"/>
<connect gate="R" pin="A" pad="A1"/>
<connect gate="R" pin="C" pad="C1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUOLED-RG-A" prefix="LD" uservalue="yes">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/green), 5 mm, round, common Anode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
<gates>
<gate name="G$1" symbol="DUOLED-RG-A"/>
</gates>
<devices>
<device name="" package="DUOLED-A-5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="CG" pad="CX"/>
<connect gate="G$1" pin="CR" pad="CR"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUOLED-RG-C" prefix="LD" uservalue="yes">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/green), 5 mm, round, common Cathode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
<gates>
<gate name="G$1" symbol="DUOLED-RG-C"/>
</gates>
<devices>
<device name="" package="DUOLED-C-5MM">
<connects>
<connect gate="G$1" pin="AG" pad="AX"/>
<connect gate="G$1" pin="AR" pad="AR"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUOLED-RY-A" prefix="LD" uservalue="yes">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/yellow), 5 mm, round, common Anode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
<gates>
<gate name="G$1" symbol="DUOLED-RY-A"/>
</gates>
<devices>
<device name="" package="DUOLED-A-5MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="CR" pad="CR"/>
<connect gate="G$1" pin="CY" pad="CX"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DUOLED-RY-C" prefix="LD" uservalue="yes">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/yellow), 5 mm, round, common Cathode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
<gates>
<gate name="G$1" symbol="DUOLED-RY-C"/>
</gates>
<devices>
<device name="" package="DUOLED-C-5MM">
<connects>
<connect gate="G$1" pin="AR" pad="AR"/>
<connect gate="G$1" pin="AY" pad="AX"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACULEDVHL" prefix="LED">
<description>&lt;b&gt;ACULED® VHL&lt;/b&gt; Standard Monochromatic and Multi-Colored Four-Chip LED&lt;p&gt;
Source: http://optoelectronics.perkinelmer.com/content/Datasheets/DTS_ACULEDVHL.pdf</description>
<gates>
<gate name="C1" symbol="LED-PAD"/>
<gate name="C2" symbol="LED-PAD"/>
<gate name="C3" symbol="LED-PAD"/>
<gate name="C4" symbol="LED-PAD"/>
</gates>
<devices>
<device name="-RGBY" package="ACULEDVHL">
<connects>
<connect gate="C1" pin="A" pad="7"/>
<connect gate="C1" pin="C" pad="8"/>
<connect gate="C2" pin="A" pad="5"/>
<connect gate="C2" pin="C" pad="6"/>
<connect gate="C3" pin="A" pad="3"/>
<connect gate="C3" pin="C" pad="4"/>
<connect gate="C4" pin="A" pad="1"/>
<connect gate="C4" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IR" package="ACULEDVHL">
<connects>
<connect gate="C1" pin="A" pad="8"/>
<connect gate="C1" pin="C" pad="7"/>
<connect gate="C2" pin="A" pad="6"/>
<connect gate="C2" pin="C" pad="5"/>
<connect gate="C3" pin="A" pad="4"/>
<connect gate="C3" pin="C" pad="3"/>
<connect gate="C4" pin="A" pad="2"/>
<connect gate="C4" pin="C" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ACULED-RGB" prefix="LED">
<description>&lt;b&gt;ACULED&lt;/b&gt;&lt;p&gt;
Source: http://optoelectronics.perkinelmer.com/content/Datasheets/DTS_ACULED.pdf</description>
<gates>
<gate name="A" symbol="ACULED-RGB"/>
</gates>
<devices>
<device name="" package="ACULED-RGB">
<connects>
<connect gate="A" pin="BA" pad="GA"/>
<connect gate="A" pin="BC" pad="BC"/>
<connect gate="A" pin="GA" pad="BA"/>
<connect gate="A" pin="GC" pad="RC"/>
<connect gate="A" pin="RA" pad="RA"/>
<connect gate="A" pin="RC" pad="GC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON_REBEL" prefix="LED">
<description>&lt;b&gt;LUXEON Rebel&lt;/b&gt;&lt;p&gt;

Display layer 93, Pins, and connect all contact points with a net.&lt;br&gt;
The thermal pads are defined in a separate gate with addlevel REQUEST.&lt;br&gt;
Draw a net named 'TH' and connect all thermal pads with it.&lt;br&gt;
Please read the Package's Description about DRC settings.&lt;p&gt;
Source: http://www.lumileds.com/pdfs/AB32.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="LUXEON_REBEL">
<connects>
<connect gate="G$1" pin="A" pad="A A@1"/>
<connect gate="G$1" pin="C" pad="C C@1"/>
<connect gate="TH" pin="TH" pad="TH TH@1 TH@2 TH@3 TH@4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LRTB_G6SG" prefix="LED">
<description>&lt;b&gt;LRTB G6SG&lt;/b&gt; 6-lead TOPLED®&lt;p&gt;
Source: OSRAM Opto Semiconductors ... LRTB_G6SG_Pb_free.pdf</description>
<gates>
<gate name="-1" symbol="LED-PAD"/>
<gate name="-2" symbol="LED-PAD"/>
<gate name="-3" symbol="LED-PAD"/>
</gates>
<devices>
<device name="" package="LRTB_G6SG">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="C" pad="6"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="C" pad="2"/>
<connect gate="-3" pin="A" pad="4"/>
<connect gate="-3" pin="C" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OVSTRGBBCR8" prefix="LED">
<description>&lt;b&gt;Full Color PLCC6 LED&lt;/b&gt; OVSTRGBBCR8&lt;p&gt;
Source: www.optekinc.com  .. ovstrgbbcr8.pdf</description>
<gates>
<gate name="-G" symbol="LED-A"/>
<gate name="-R" symbol="LED-A"/>
<gate name="G$1" symbol="LED-A"/>
</gates>
<devices>
<device name="" package="OVSTRGBBCR8">
<connects>
<connect gate="-G" pin="A" pad="1"/>
<connect gate="-G" pin="C" pad="4 4@1" route="any"/>
<connect gate="-R" pin="A" pad="2"/>
<connect gate="-R" pin="C" pad="5 5@1" route="any"/>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="6 6@1" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2C63-ST-RGB-SR0" prefix="LED">
<description>&lt;b&gt;1.5W RGB HIGH POWER LED&lt;/b&gt;&lt;p&gt;
Source: http://www.ledtech.com.tw .. LP2C63-ST-RGB-SR0.SPEC.pdf</description>
<gates>
<gate name="G" symbol="LED"/>
<gate name="R" symbol="LED"/>
<gate name="B" symbol="LED"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="LP2C63-ST-RGB-SR0">
<connects>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="C" pad="4"/>
<connect gate="G" pin="A" pad="1"/>
<connect gate="G" pin="C" pad="6"/>
<connect gate="R" pin="A" pad="2"/>
<connect gate="R" pin="C" pad="5"/>
<connect gate="TH" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*W57B" prefix="LED">
<description>&lt;b&gt;Golden Dragon® 1 Watt LED&lt;/b&gt;&lt;p&gt;
Place heat sink pads of cathode with INVOKE&lt;br&gt;
Source: www.osram-os.com la_ly_w57b.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="W57B">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C C@1 C@2 C@3 C@4 C@5"/>
</connects>
<technologies>
<technology name="LA"/>
<technology name="LY"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="?W5KM" prefix="LED">
<description>&lt;b&gt;Golden DRAGON® ARGUS® LED&lt;/b&gt;&lt;p&gt;
Place TH-Gate and connect pins in schematic.&lt;br&gt;
Set DRC-Clearance - Same Signals to 0mm in board.&lt;br&gt;
Source: catalog.osram-os.com .. LD_LB_LT_W5KM_Pb_free.pdf</description>
<gates>
<gate name="G$1" symbol="LED+D"/>
<gate name="G$2" symbol="THERMAL"/>
</gates>
<devices>
<device name="LB" package="W5KM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$2" pin="TH" pad="HT@1 HT@2 TH"/>
</connects>
<technologies>
<technology name="-EZGY-35">
<attribute name="COLOR" value="blue"/>
</technology>
</technologies>
</device>
<device name="LD" package="W5KM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$2" pin="TH" pad="HT@1 HT@2 TH"/>
</connects>
<technologies>
<technology name="-1S2T-35">
<attribute name="COLOR" value="deep blue"/>
</technology>
</technologies>
</device>
<device name="LT" package="W5KM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$2" pin="TH" pad="HT@1 HT@2 TH"/>
</connects>
<technologies>
<technology name="-HZKX-25">
<attribute name="COLOR" value="true green"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*_T679-?-1" prefix="LED">
<description>&lt;b&gt;LC TOPLED® Low Current LED&lt;/b&gt;&lt;p&gt;
Source: http://catalog.osram-os.com .. LG_LS_LY_T679_OBS.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="D2E2" package="PLCC2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="LS">
<attribute name="COLOR" value="super-red"/>
</technology>
<technology name="LY">
<attribute name="COLOR" value="yellow"/>
</technology>
</technologies>
</device>
<device name="E1F1" package="PLCC2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="LG">
<attribute name="COLOR" value="green"/>
</technology>
</technologies>
</device>
<device name="F1G2" package="PLCC2">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="LG">
<attribute name="COLOR" value="green"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*W51M" prefix="LED">
<description>&lt;b&gt;Golden DRAGON® with Lens&lt;/b&gt; Enhanced Thinfilm LED&lt;p&gt;
Source: LA_LR_LY_W51M_Pb_free[1].pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="G$2" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="W51">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$2" pin="TH" pad="TH@1 TH@2 TH@3" route="any"/>
</connects>
<technologies>
<technology name="LA"/>
<technology name="LR"/>
<technology name="LY"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*W51M-TH" prefix="LED">
<description>&lt;b&gt;Golden DRAGON® with Lens&lt;/b&gt; Enhanced Thinfilm LED&lt;p&gt;
Source: LA_LR_LY_W51M_Pb_free[1].pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="G$2" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="W51-COOL">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$2" pin="TH" pad="TH@1 TH@2 TH@3 TH@4 TH@5 TH@6 TH@7 TH@8 TH@9 TH@10 TH@11 TH@12"/>
</connects>
<technologies>
<technology name="LA"/>
<technology name="LR"/>
<technology name="LY"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GM1BW78140A" prefix="LED">
<description>&lt;b&gt;High Brightness Chip LED (White)&lt;/b&gt; 39 lm @ 150 mA&lt;p&gt;
Source: http://document.sharpsma.com/files/GM1BW78140A.pdf</description>
<gates>
<gate name="G$1" symbol="LED4P"/>
</gates>
<devices>
<device name="" package="GM1BW78140A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GM1BW76340A" prefix="LED">
<description>&lt;b&gt;White LED&lt;/b&gt; 45 lumen 14000 mcd @50 mA&lt;p&gt;
http://document.sharpsma.com/files/GM1BW76340A_DS.pdf</description>
<gates>
<gate name="G$1" symbol="LED-4"/>
</gates>
<devices>
<device name="" package="GM1BW78140A">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GM1WA55311A" prefix="LED">
<description>&lt;b&gt;Chip LED RGB&lt;/b&gt;&lt;p&gt;
Source: http://document.sharpsma.com/files/GM1WA55311A_SS.pdf</description>
<gates>
<gate name="G$1" symbol="LED-RGB-A"/>
</gates>
<devices>
<device name="" package="GM1WA55311A">
<connects>
<connect gate="G$1" pin="A" pad="4"/>
<connect gate="G$1" pin="CBLUE" pad="3"/>
<connect gate="G$1" pin="CGREEN" pad="1"/>
<connect gate="G$1" pin="CRED" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GM5WA94310A" prefix="LED">
<description>&lt;b&gt;Chip LED&lt;/b&gt; RGB&lt;p&gt;
Source: http://document.sharpsma.com/files/GM5WA94310A_SS.pdf</description>
<gates>
<gate name="R" symbol="LED"/>
<gate name="G" symbol="LED"/>
<gate name="B" symbol="LED"/>
</gates>
<devices>
<device name="" package="GM5WA94310A">
<connects>
<connect gate="B" pin="A" pad="1"/>
<connect gate="B" pin="C" pad="6"/>
<connect gate="G" pin="A" pad="3"/>
<connect gate="G" pin="C" pad="4"/>
<connect gate="R" pin="A" pad="2"/>
<connect gate="R" pin="C" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GM5BW96385A" prefix="LED">
<description>&lt;b&gt;High brightness White Color LED&lt;/b&gt; 2300 mcd @ IF = 20mA&lt;p&gt;
achieved via InGaN Blue LED chip in combination with Yellow Phosphor&lt;br&gt;
Source: http://document.sharpsma.com/files/GM5BW96385A.pdf</description>
<gates>
<gate name="B" symbol="LED+D"/>
</gates>
<devices>
<device name="" package="GM5BW96385A">
<connects>
<connect gate="B" pin="A" pad="A"/>
<connect gate="B" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NSSM038A" prefix="LED">
<description>&lt;b&gt;NICHIA CHIP TYPE FULL COLOR LED&lt;/b&gt;&lt;p&gt;
Source: NICIA CORPORATION .. NSSM038AT-E.PDF</description>
<gates>
<gate name="B" symbol="NSSM038A-RGB"/>
</gates>
<devices>
<device name="" package="NSSM038A">
<connects>
<connect gate="B" pin="BA" pad="1"/>
<connect gate="B" pin="BC" pad="2 2@1"/>
<connect gate="B" pin="GA" pad="6"/>
<connect gate="B" pin="GC" pad="5 5@1"/>
<connect gate="B" pin="RA" pad="3"/>
<connect gate="B" pin="RC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W724C0" prefix="LED">
<description>&lt;b&gt;Z-Power LED&lt;/b&gt; P7 Series&lt;p&gt;
Source: http://www.acriche.com .. W724C0.pdf</description>
<gates>
<gate name="G$1" symbol="LED4-A2C2"/>
<gate name="G$2" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="W724C0">
<connects>
<connect gate="G$1" pin="A" pad="A@1 A@2"/>
<connect gate="G$1" pin="C" pad="C@1 C@2"/>
<connect gate="G$2" pin="TH" pad="TH@1 TH@2 TH@3 TH@4 TH@5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="F50360" prefix="LED">
<description>&lt;b&gt;Full color Z-Power LED RGB&lt;/b&gt; P5-II Series&lt;p&gt;
Source: http://www.seoulsemicon.co.kr .. F50360.pdf</description>
<gates>
<gate name="G$1" symbol="LED-RGB-D"/>
</gates>
<devices>
<device name="" package="F50360">
<connects>
<connect gate="G$1" pin="BA" pad="BA"/>
<connect gate="G$1" pin="BC" pad="BC"/>
<connect gate="G$1" pin="GA" pad="GA"/>
<connect gate="G$1" pin="GC" pad="GC"/>
<connect gate="G$1" pin="RA" pad="RA"/>
<connect gate="G$1" pin="RC" pad="RC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="X42180" prefix="LED">
<description>&lt;b&gt;Z-Power LED&lt;/b&gt; P4 Series, Dome type&lt;p&gt;
Source: http://www.seoulsemicon.co.kr .. X42180.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="Z-POWER-LED-DOME-TYPE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="X42182" prefix="LED">
<description>&lt;b&gt;Z-Power LED&lt;/b&gt; P4 Series, Dome type&lt;/b&gt;&lt;p&gt;
Source: http://www.seoulsemicon.co.kr .. X42182.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="Z-POWER-LED-DOME-TYPE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="W49180" prefix="LED">
<description>&lt;b&gt;Z-Power LED&lt;/b&gt; P4 Series, Dome type&lt;p&gt;
Source: http://www.acriche.com .. W49180.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="Z-POWER-LED-DOME-TYPE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZC-00CW40" prefix="LED">
<description>&lt;b&gt;High Luminous Efficacy Cool White LED Emitter&lt;/b&gt;&lt;p&gt;
Source: http://www.ledengin.com/products/40wLZ/LZC-00CW40.pdf</description>
<gates>
<gate name="G$1" symbol="LED-2X6"/>
</gates>
<devices>
<device name="" package="LZC-00CW40">
<connects>
<connect gate="G$1" pin="A1" pad="14 15"/>
<connect gate="G$1" pin="A2" pad="17 18"/>
<connect gate="G$1" pin="C1" pad="5 6"/>
<connect gate="G$1" pin="C2" pad="2 3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZ1-00WW03" prefix="LED">
<description>&lt;b&gt;High Luminous Efficacy 3W Warm White LED Emitter&lt;/b&gt;&lt;p&gt;
Source: http://www.ledengin.com/products/3wLZ/LZ1-00WW03.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LZ1-00WW03">
<connects>
<connect gate="G$1" pin="A" pad="2 3 5"/>
<connect gate="G$1" pin="C" pad="1 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZ1-00WW05" prefix="LED">
<description>&lt;b&gt;High Luminous Efficacy 5W Warm White LED&lt;/b&gt;&lt;p&gt;
Source: http://www.ledengin.com/products/5wLZ/LZ1-00WW05.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LZ1-00WW03">
<connects>
<connect gate="G$1" pin="A" pad="2 3 5"/>
<connect gate="G$1" pin="C" pad="1 4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZ4-00WW10" prefix="LED">
<description>&lt;b&gt;High Luminous Efficacy 10W LED&lt;/b&gt;&lt;p&gt;
http://www.ledengin.com/products/10wLZ/LZ4-00WW10.pdf</description>
<gates>
<gate name="C" symbol="LED-A"/>
<gate name="D" symbol="LED-A"/>
<gate name="A" symbol="LED-A"/>
<gate name="B" symbol="LED-A"/>
</gates>
<devices>
<device name="" package="LZ4-00WW10">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="B" pin="A" pad="3 4"/>
<connect gate="B" pin="C" pad="9"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="C" pad="6"/>
<connect gate="D" pin="A" pad="7"/>
<connect gate="D" pin="C" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XPEWHT-" prefix="LED">
<description>&lt;b&gt;Cree® XLamp® XP-E LEDs&lt;/b&gt;&lt;p&gt;
Source: www.cree.com/xlamp .. XLampXP-E.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="CREE_XLAMP">
<connects>
<connect gate="G$1" pin="A" pad="A A@1"/>
<connect gate="G$1" pin="C" pad="C C@1"/>
</connects>
<technologies>
<technology name="01-0000-00BC2"/>
<technology name="01-0000-00CC2"/>
<technology name="01-0000-00DC2"/>
<technology name="01-0000-00EC2"/>
<technology name="L1-0000-007E7"/>
<technology name="L1-0000-008E7"/>
<technology name="L1-0000-009E4"/>
<technology name="L1-0000-009E7"/>
<technology name="L1-0000-00AE4"/>
<technology name="L1-0000-00AE7"/>
<technology name="L1-0000-00B01"/>
<technology name="L1-0000-00BE4"/>
<technology name="L1-0000-00C01"/>
<technology name="L1-0000-00CE4"/>
<technology name="L1-0000-00D01"/>
<technology name="L1-0000-00E01"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L-115WEGW-CA" prefix="LED">
<description>&lt;b&gt;T-1(3mm) BI-COLOR INDICATOR LAMP&lt;/b&gt;&lt;p&gt;
Source: Kingbright .. 2_colour_led_.pdf</description>
<gates>
<gate name="G$1" symbol="DUOLED-RG-A"/>
</gates>
<devices>
<device name="" package="DUOLED-A-3MM">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="CG" pad="1"/>
<connect gate="G$1" pin="CR" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLUV5300" prefix="LED">
<description>&lt;b&gt;Bicolor LED 5 mm&lt;/b&gt; Untinted Diffused Package&lt;p&gt;
Source: www.vishay.com .. Bi-Color LED Vashay TLUV5300.pdf</description>
<gates>
<gate name="G$1" symbol="DUOLED-OG-C"/>
</gates>
<devices>
<device name="" package="TLUV5300">
<connects>
<connect gate="G$1" pin="AG" pad="AG"/>
<connect gate="G$1" pin="AO" pad="AO"/>
<connect gate="G$1" pin="CC" pad="CC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*P4" prefix="LED">
<description>&lt;b&gt;PointLED® Enhanced Thinfilm LED&lt;/b&gt; TOP &amp; BOTTOM mount&lt;p&gt;
LS P47F, LR P47F, LA P47F, LY P47F, LT P4SG, LB P4SG, LW P4SG&lt;br&gt;
Source: http://catalog.osram-os.com .. LA_LR_LS_LY_P47F_Pb_free.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="-BOTTOM" package="P47F-BOTTOM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="LA"/>
<technology name="LB"/>
<technology name="LR"/>
<technology name="LS"/>
<technology name="LT"/>
<technology name="LW"/>
<technology name="LY"/>
</technologies>
</device>
<device name="-TOP" package="P47F-TOP">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="LA"/>
<technology name="LB"/>
<technology name="LR"/>
<technology name="LS"/>
<technology name="LT"/>
<technology name="LW"/>
<technology name="LY"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L-59EGW-CA" prefix="LED">
<description>&lt;b&gt;T-1 3/4 (5mm) BI-COLOR INDICATOR LAMP&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/L-59EGW-CA%28Ver1292805989.13%29</description>
<gates>
<gate name="G$1" symbol="DUOLED-RG-A"/>
</gates>
<devices>
<device name="" package="L-59EGW-CA">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="CG" pad="3"/>
<connect gate="G$1" pin="CR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLLY4400" prefix="LED">
<description>&lt;b&gt;Low Current (2mA) LED 3 mm Tinted Diffused Package&lt;/b&gt; color&lt;b&gt;&lt;font color="#909020"&gt; YELLOW&lt;/font&gt;&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.farnell.com/datasheets/391098.pdf"&gt; Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="VISHAY SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="1612439"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLLR4400" prefix="LED">
<description>&lt;b&gt;Low Current (2mA) LED 3 mm Tinted Diffused Package&lt;/b&gt; color &lt;b&gt;&lt;font color="darkred"&gt;RED&lt;/font&gt;&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.farnell.com/datasheets/391100.pdf"&gt; Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="VISHAY SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="1612437"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLLG4400" prefix="LED">
<description>&lt;b&gt;Low Current (2mA) LED 3 mm Tinted Diffused Package&lt;/b&gt; color &lt;b&gt;&lt;font color="green"&gt;GREEN&lt;/font&gt;&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.farnell.com/datasheets/391098.pdf"&gt; Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LED3MM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="VISHAY SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="1612435"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CLN6A" prefix="LED">
<description>&lt;b&gt;Cree® CLN6A-WKW/MKW LED&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/LEDlamps/CLN6A%28979%29.pdf"&gt; Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="CLN6A">
<connects>
<connect gate="G$1" pin="A" pad="4 5 6"/>
<connect gate="G$1" pin="C" pad="1 2 3"/>
<connect gate="TH" pin="TH" pad="HT"/>
</connects>
<technologies>
<technology name="-MKW"/>
<technology name="-WKW"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="Z-POWER-LED" prefix="LED">
<description>&lt;b&gt;Z-Power LED&lt;/b&gt;&lt;p&gt;
Source: http://www.seoulsemicon.co.kr .. X42182.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="Z-POWER-LED-PCB-TYPE">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PB3XX301V050A" prefix="LED">
<description>&lt;b&gt;Self-addressed led , single point control with integrated RGB leds and drive IC&lt;/b&gt;&lt;p&gt;
Easy control by MCU.&lt;br&gt;
Source: DycolED.pdf &lt;a href="http://www.kirronlightcomponents.com/index.php/download_file/view/41/83/"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="PB3XX301V050A"/>
</gates>
<devices>
<device name="" package="PB3XX301V050A">
<connects>
<connect gate="G$1" pin="CI" pad="2"/>
<connect gate="G$1" pin="CO" pad="5"/>
<connect gate="G$1" pin="DI" pad="1"/>
<connect gate="G$1" pin="DO" pad="4"/>
<connect gate="G$1" pin="VDD" pad="6"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX6" prefix="LED">
<description>&lt;b&gt;Cree® XLamp® MX-6 LEDs&lt;/b&gt; with cooling drills for FR4&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/XLampMX-6.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="B" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="MX6">
<connects>
<connect gate="B" pin="TH" pad="TH TH@1 TH@2 TH@3 TH@4 TH@5 TH@6 TH@7 TH@8 TH@9 TH@10 TH@11 TH@12 TH@13 TH@14" route="any"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX3" prefix="LED">
<description>&lt;b&gt;Cree® XLamp® MX-3 LEDs&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/XLampMX-3.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="B" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="MX6">
<connects>
<connect gate="B" pin="TH" pad="TH TH@1 TH@2 TH@3 TH@4 TH@5 TH@6 TH@7 TH@8 TH@9 TH@10 TH@11 TH@12 TH@13 TH@14"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MX6-ALU" prefix="LED">
<description>&lt;b&gt;Cree® XLamp® MX-6 LEDs&lt;/b&gt; for mounting on ALU PCBs&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/XLampMX-6.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="MX6-ALU">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SPHWHTHAD605S0W0U4" prefix="LED">
<description>&lt;b&gt;HV-AC HIGH POWER LED&lt;/b&gt;&lt;p&gt;
Source: SAMSUNG SPHWHTHAD605S0W0U4.pdf</description>
<gates>
<gate name="G$1" symbol="SPHWHTHAD605S0W0U4"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="SPHWHTHAD605S0W0U4">
<connects>
<connect gate="G$1" pin="1" pad="1 1@1" route="any"/>
<connect gate="G$1" pin="2" pad="2 2@1" route="any"/>
<connect gate="G$1" pin="4" pad="4 4@1" route="any"/>
<connect gate="G$1" pin="5" pad="5 5@1" route="any"/>
<connect gate="TH" pin="TH" pad="3 3@1 3@2 3@3 3@4 3@5" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ML-E" prefix="LED">
<description>&lt;b&gt;Cree® XLamp® ML-E LEDs&lt;/b&gt; 1/2 watt, 3.5 x 3.5 mm&lt;p&gt;
Source: &lt;a href="http://www.cree.com/products/pdf/XLampML-E.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LED-A2C2"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="ML-E">
<connects>
<connect gate="G$1" pin="A@1" pad="A@1"/>
<connect gate="G$1" pin="A@2" pad="A@2"/>
<connect gate="G$1" pin="C@1" pad="C@1"/>
<connect gate="G$1" pin="C@2" pad="C@2"/>
<connect gate="TH" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CREE-XLAMP-XM-L" prefix="LED">
<description>&lt;b&gt;Cree® XLamp® XM-L LEDs&lt;/b&gt;&lt;p&gt;
Source: http://www.cree.com</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="CREE-XLAMP-XM-L">
<connects>
<connect gate="G$1" pin="A" pad="A A@1"/>
<connect gate="G$1" pin="C" pad="C C@1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LSG-T676" prefix="LED">
<description>&lt;b&gt;LSG T676 Hyper Multi TOPLED ® Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
Source: http://docs-europe.electrocomponents.com/webdocs/08c3/0900766b808c36ca.pdf</description>
<gates>
<gate name="A" symbol="LED"/>
<gate name="B" symbol="LED"/>
</gates>
<devices>
<device name="COOL" package="P-LCC4-T676">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="B" pin="A" pad="4"/>
<connect gate="B" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="P-LCC4-0">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="B" pin="A" pad="4"/>
<connect gate="B" pin="C" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LZ4-40U600" prefix="LED">
<description>&lt;b&gt;High Efficacy 365nm UV LED Emitter&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ledengin.com/files/products/LZ4/LZ4-00U600.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="A" symbol="LED"/>
<gate name="B" symbol="LED"/>
<gate name="C" symbol="LED"/>
<gate name="D" symbol="LED"/>
</gates>
<devices>
<device name="" package="LZ4-40U600">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="C" pad="2"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="C" pad="4"/>
<connect gate="C" pin="A" pad="5"/>
<connect gate="C" pin="C" pad="6"/>
<connect gate="D" pin="A" pad="7"/>
<connect gate="D" pin="C" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUXEON_5630" prefix="LED">
<description>&lt;b&gt;LUXEON 5630 Mid-Power LEDs&lt;/b&gt; SD201&lt;p&gt;
Source: &lt;a href="www.philipslumileds.com/uploads/351/DS201-pdf"&gt; Data sheet &lt;/a&gt;&lt;br&gt;
Lumileds 5630 Datasheet DS201 20130228 ©2013 Philips Lumileds Lighting Company.</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LUXEON_5630">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1@1 1@2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PC56H19_V0" prefix="LED">
<description>&lt;b&gt;Lextar&lt;/b&gt; white SMD LED&lt;p&gt;
Source: PC56H19_20150317.pdf&lt;br&gt;
www.lextar.com</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="PC56H19_V0">
<connects>
<connect gate="G$1" pin="A" pad="2 4"/>
<connect gate="G$1" pin="C" pad="1 3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
