<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.3">
<drawing>
<library>
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
<package name="TO18">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="TO39">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="SIP11">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
11 lead, National Semiconductor</description>
</package>
<package name="TO78">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="TO99">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="TO100">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="CB360">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt; 5 lead</description>
</package>
<package name="CB367">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;5 lead</description>
</package>
<package name="TO39/4">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="PGA68">
<description>&lt;b&gt;Pin Grid Array&lt;/b&gt;&lt;p&gt;68 lead</description>
</package>
<package name="TO78H">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;</description>
</package>
<package name="H03A">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;&lt;p&gt;
National Semiconductor NS H03A&lt;br&gt;
Motorola MOT 79-05</description>
</package>
<package name="H03B">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;&lt;p&gt;
National Semiconductor H03B</description>
</package>
<package name="H08C">
<description>&lt;b&gt;TO-99&lt;/b&gt;&lt;p&gt;
National Semiconductor H08C&lt;br&gt;
Motorola MOT 601-04</description>
</package>
<package name="H10C">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;&lt;p&gt;
National Semiconductor NS H10C&lt;br&gt;
Motorola  603-04 / 603C-01</description>
</package>
<package name="HA04E">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;&lt;p&gt;
National Semiconductor HA04E</description>
</package>
<package name="TO3">
<description>&lt;b&gt;Metal Can Package&lt;/b&gt;&lt;p&gt;
MOTOROLA 1-03</description>
</package>
<package name="K02A">
<description>&lt;b&gt;TO-3&lt;/b&gt;&lt;p&gt;
National Semiconductor K02A</description>
</package>
<package name="K02B">
<description>&lt;b&gt;TO-3&lt;/b&gt;&lt;p&gt;
National Semiconductor K02B</description>
</package>
<package name="K04A">
<description>&lt;b&gt;TO-3&lt;/b&gt;&lt;p&gt;
National Semiconductor K04A</description>
</package>
<package name="K08A">
<description>&lt;b&gt;TO-3&lt;/b&gt;&lt;p&gt;
National Semiconductor K08A</description>
</package>
<package name="KC02A">
<description>&lt;b&gt;TO-3&lt;/b&gt;&lt;p&gt;
National Semiconductor KC02A</description>
</package>
<package name="KA15A">
<description>&lt;b&gt;TO-3&lt;/b&gt;&lt;p&gt;
National Semiconductor KA15A</description>
</package>
<package name="P03A">
<description>&lt;b&gt;TO-202&lt;/b&gt;&lt;p&gt;
National Semiconductor P03A</description>
</package>
<package name="P04A">
<description>&lt;b&gt;TO-202&lt;/b&gt;&lt;p&gt;
National Semiconductor P04A</description>
</package>
<package name="T03B">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
3 lead, National Semiconductor T03A T03B&lt;br&gt;
Motorola 221A-04</description>
</package>
<package name="T05A">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
5 lead, National Semiconductor T05A&lt;br&gt;
Motorola 314D-01</description>
</package>
<package name="T05D">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
5 lead, National Semiconductor T05D</description>
</package>
<package name="TA11B">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
11 lead, National Semiconductor TA11B</description>
</package>
<package name="TA15A">
<description>&lt;b&gt;TO-220&lt;/b&gt;&lt;p&gt;
15 lead, National Semiconductor TA15A</description>
</package>
<package name="Z03A">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
National Semiconductor Z03A</description>
</package>
<package name="PLCC20S">
<description>&lt;b&gt;PLCC&lt;/b&gt;&lt;p&gt;
20 lead square</description>
</package>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package 16&lt;/b&gt; large</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="TSSOP8">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 8&lt;/b&gt; 3 x 4.4 mm&lt;p&gt;</description>
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;</description>
</package>
<package name="TO263-5">
<description>&lt;b&gt;TO-263&lt;/b&gt;</description>
</package>
<package name="TO220-51">
<description>&lt;b&gt;TO-220&lt;/b&gt; P-TO220-5/1</description>
</package>
<package name="TO220-52">
<description>&lt;b&gt;TO-220&lt;/b&gt; P-TO220-5-2&lt;p&gt;
SIEMENS TLE4270</description>
</package>
<package name="SO14W">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt; wide</description>
</package>
<package name="SO20W">
<description>&lt;b&gt;Small Outline Package 20&lt;/b&gt; wide</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline Package 16&lt;/b&gt;</description>
</package>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
<package name="DPACK_1">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 1 (Motorola)</description>
</package>
<package name="DPACK_2">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 2 (Motorola)</description>
</package>
<package name="DPACK_3">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 3 (Motorola)</description>
</package>
<package name="DPACK_4">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 4 (Motorola)</description>
</package>
<package name="DPACK_5">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 5 (Motorola)</description>
</package>
<package name="DPACK_6">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 6 (Motorola)</description>
</package>
<package name="SO28W">
<description>&lt;b&gt;Small Outline Package 28&lt;/b&gt; wide</description>
</package>
<package name="SO24W">
<description>&lt;b&gt;Small Outline Package 24&lt;/b&gt; wide</description>
</package>
<package name="PLCC28S">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="MULTIWAT-SIL17">
<description>&lt;b&gt;DBS17P&lt;/b&gt; plastic DIL-bent-SIL power package&lt;p&gt;
17 leads (lead length 12 mm) SOT243-1</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL10">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="MULTIWAT-SIL13">
<description>&lt;b&gt;DBS13P&lt;/b&gt; plastic DIL-bent-SIL power package&lt;p&gt;
13 leads (lead length 12 mm) SOT141-6&lt;br&gt;
Source: TDA1516BQ_1.pdf</description>
</package>
<package name="TO46">
<description>&lt;b&gt;NS Package H03H&lt;/b&gt;</description>
</package>
<package name="ZIP21-SLA">
<description>&lt;b&gt;Small molded power package&lt;/b&gt; ZIP-type 21-pin SLA package&lt;p&gt;
Source: www.allegromicro.com .. 97060.pdf</description>
</package>
<package name="TO263-3">
<description>&lt;b&gt;TO-263 3-Lead Plastic Surface Mount Package&lt;/b&gt; NS Package Number TS3B&lt;p&gt;
Source. http://cache.national.com/ds/LM/LM2937-2.5.pdf</description>
</package>
<package name="TQFP52">
<description>&lt;b&gt;TQFP-52&lt;/b&gt; PLASTIC PACKAGE CASE 848B-04&lt;p&gt;
Source: www.motorola.com .. MC33215.pdf</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
(Motorola)</description>
</package>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="HSIP17-P-2.00">
<description>&lt;b&gt;HSIP17-P-2.00&lt;/b&gt;&lt;p&gt;
Source: http://www.semicon.toshiba.co.jp/td/en/ASSP/Audio_ICs/en_20050517_TA8210ALQ_datasheet.pdf</description>
</package>
<package name="HZIP17-P-2.00">
<description>&lt;b&gt;HZIP17-P-2.00&lt;/b&gt;&lt;p&gt;
Source: http://www.semicon.toshiba.co.jp/td/en/ASSP/Audio_ICs/en_20050517_TA8210ALQ_datasheet.pdf</description>
</package>
<package name="SIP-12">
<description>&lt;b&gt;12-Lead SIL Platic Package with Fin (12-SIP-FP)&lt;/b&gt;&lt;p&gt;
Source: http://www.steren.com.mx/diagramas/uploads/an7161.pdf</description>
</package>
<package name="TO3-8">
<description>&lt;b&gt;8-PIN TO-3&lt;/b&gt;&lt;p&gt;
Source: http://eportal.apexmicrotech.com/mainsite/pdf/CE.pdf</description>
</package>
<package name="MSOP08">
<description>&lt;b&gt;Mini Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="SIP-10">
<description>&lt;b&gt;10-Pin Ceramic SIP&lt;/b&gt;&lt;p&gt;
Source: http://eportal.apexmicrotech.com/mainsite/pdf/DW.pdf</description>
</package>
<package name="PSOP24">
<description>&lt;b&gt;24-PIN PSOP&lt;/b&gt; (JEDEC MO-166)&lt;p&gt;
Source: http://eportal.apexmicrotech.com/mainsite/pdf/DF.pdf</description>
</package>
<package name="LF871">
<description>&lt;b&gt;18-pin single in-line power-tab package&lt;/b&gt; LF871&lt;p&gt;
Source: //www.allegromicro.com/datafile/97052.pdf</description>
</package>
<package name="LF872">
<description>&lt;b&gt;18-pin single in-line power-tab package&lt;/b&gt; LF872&lt;p&gt;
Source: http://www.allegromicro.com/datafile/97052.pdf</description>
</package>
<package name="WW">
<description>&lt;b&gt;Plastic Micro-X WW&lt;/b&gt;&lt;p&gt;
Source: http://www.minicircuits.com/dwgs/outline_drawings.pdf</description>
</package>
<package name="VV">
<description>&lt;b&gt;Plastic Micro-X  VV&lt;/b&gt;&lt;p&gt;
Source: http://www.minicircuits.com/dwgs/outline_drawings.pdf</description>
</package>
<package name="SO16DW">
<description>&lt;b&gt;SOIC 16 DW SUFFIX&lt;/b&gt; PLASTIC SOIC PACKAGE CASE 751G-03 ISSUE B&lt;p&gt;
http://www.onsemi.com/pub/Collateral/MC14536B-D.PDF</description>
</package>
<package name="SO16W">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
wide body 7.5 mm/JEDEC MS-013AA</description>
</package>
<package name="SO16-F">
<description>&lt;b&gt;SOEIAJ-16 F SUFFIX&lt;/b&gt; PLASTIC EIAJ SOIC PACKAGE CASE 966-01 ISSUE O&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC14536B-D.PDF</description>
</package>
<package name="SO18W300">
<description>&lt;b&gt;18-Lead Plastic Small Outline (SO) - Wide, 300 mil (SOIC)&lt;/b&gt;&lt;p&gt;
Source: http://www.rfsolutions.co.uk/acatalog/DS601-4.pdf</description>
</package>
<package name="UDN2954W">
<description>&lt;b&gt;SIP 12&lt;/b&gt;&lt;p&gt;
Source: http://allegromicro.com/datafile/archive/2953.pdf</description>
</package>
<package name="PLCC-S44">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt; Socked</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="TSSOP28">
<description>&lt;b&gt;LP Package, 28-Pin TSSOP with Exposed Thermal Pad&lt;/b&gt;&lt;p&gt;
Source: http://allegromicro.com/datafile/3979.pdf</description>
</package>
<package name="TMD09AAA">
<description>&lt;b&gt;THIN MICRO SMD, 9 BUMP, 0.4mm PITCH&lt;/b&gt; 1.22 x 1.22 x 0.60mm body size&lt;p&gt;
Source: http://www.national.com/packaging/mkt/tmd09xxx.pdf</description>
</package>
<package name="TO-226AA">
<description>&lt;b&gt;TO-226AA&lt;/b&gt; P SUFFIX, CASE 29-11&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF</description>
</package>
<package name="TSOP-5">
<description>&lt;b&gt;TSOP-5&lt;/b&gt; PLASTIC PACKAGE CASE 483-02&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF</description>
</package>
<package name="SOIC8">
<description>&lt;b&gt;SOIC-8&lt;/b&gt; CASE 751-07&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF&lt;p&gt;
&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;PLATIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
</package>
<package name="MICRO8">
<description>&lt;b&gt;Micro8&lt;/b&gt; CASE 846A-02&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF</description>
</package>
<package name="PSOP08">
<description>&lt;b&gt;PS (R-PDSO-G8)&lt;/b&gt; PLATIC SMALL-OUTLINE-PACKAGE&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
</package>
<package name="MMSOP08">
<description>&lt;b&gt;Molded Mini Small Outline Package&lt;/b&gt; 8 - Lead (0.118" Wide)&lt;p&gt;
NS Package Number MUA08A&lt;br&gt;
Source: http://cache.national.com/ds/LM/LM386.pdf</description>
</package>
<package name="SOT89">
<description>&lt;b&gt;SOT98&lt;/b&gt; PK (R-PDSO-G3)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78l05.pdf</description>
</package>
<package name="SC70-5L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="0804MC">
<description>&lt;b&gt;TO3-8 Socket&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/0804mc.pdf</description>
</package>
<package name="DFN8-4X4">
<description>&lt;b&gt;DFN8 4x4 mm&lt;/b&gt; DRM (S-PDSO-N8)&lt;p&gt;
Source: opa277.pdf</description>
</package>
<package name="SIP8">
<description>&lt;b&gt;Single Inline Palstic Package 8 pol.&lt;/b&gt;&lt;p&gt;
Source: ROHM BA728.pdf</description>
</package>
<package name="MSOP10">
<description>&lt;b&gt;10 Lead MSOP Package&lt;/b&gt; NS Package Number MUB10A&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM5030.pdf</description>
</package>
<package name="LLP10">
<description>&lt;b&gt;10 Lead LLP Package&lt;/b&gt; NS Package Number SDC10A&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM5030.pdf</description>
</package>
<package name="SSOP16">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 16&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
<package name="SIP8-DQ">
<description>&lt;b&gt;8 PIN SIP Style DQ&lt;/b&gt;&lt;p&gt;
Source: www.apexmicrotech.com .. DQ.pdf</description>
</package>
<package name="SOT23-6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; 6 lead</description>
</package>
<package name="SIP9-P-2.54A">
<description>&lt;b&gt;SIP9-P-2.54A&lt;/b&gt;&lt;p&gt;
Source: THOSHIBA .. TA7358P.pdf</description>
</package>
<package name="D_R-PDSO-G8">
<description>&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slos063b/slos063b.pdf</description>
</package>
<package name="PS_R-PDSO-G8">
<description>&lt;b&gt;PS (R-PDSO-G8)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slos063b/slos063b.pdf</description>
</package>
<package name="LCCC28">
<description>&lt;b&gt;FK (S-CQCC-N28)&lt;/b&gt; LEADLESS CERAMIC CHIP CARRIER&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slos063b/slos063b.pdf</description>
</package>
<package name="LCCC20">
<description>&lt;b&gt;FK (S-CQCC-N20)&lt;/&lt;LEADLEES CERAMIC CHIP CARRIER&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slos063b/slos063b.pdf</description>
</package>
<package name="DBV-R-PDSO-G5">
<description>&lt;b&gt;DBV (R-PDSO-G5)&lt;/b&gt; PLASTIC SMALL-OUTLINE PACKAGE&lt;p&gt;
Source: http://www.ti.com .. tl331.pdf</description>
</package>
<package name="TSSOP14-RU">
<description>&lt;b&gt;14-Lead Thin Shrink Small Outline Package&lt;/b&gt; [TSSOP] (RU-14)&lt;p&gt;
Source: www.analog.com .. OP1177_2177_4177.pdf</description>
</package>
<package name="SSOP14">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="2NUL2CMP">
<pin name="ON/CMP" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="ON" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="CMP" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="2CMP">
<pin name="CMP1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="CMP2" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="2NUL">
<pin name="ON2" direction="pas"/>
<pin name="ON1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="OPT" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="LH0002">
<pin name="V2+" direction="in"/>
<pin name="V1+" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="V1-" direction="in"/>
<pin name="V2-" direction="in"/>
<pin name="E4"/>
<pin name="OUT" direction="out"/>
<pin name="E3"/>
</symbol>
<symbol name="LH0004">
<pin name="CMP1" direction="pas"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="CMP2" direction="pas"/>
<pin name="BS2"/>
<pin name="BS1"/>
<pin name="OUT" direction="out"/>
<pin name="CMP1/CL" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="LM3900">
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="-IN" direction="in"/>
</symbol>
<symbol name="555">
<pin name="TR" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="R" direction="in" function="dot"/>
<pin name="CV" direction="in"/>
<pin name="THR" direction="in"/>
<pin name="DIS" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="78XX">
<pin name="VI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="pas"/>
</symbol>
<symbol name="79XX">
<pin name="VI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="pas"/>
</symbol>
<symbol name="317">
<pin name="VI" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="VO" direction="pas"/>
</symbol>
<symbol name="337">
<pin name="VI" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="VO" direction="pas"/>
</symbol>
<symbol name="PWR+G">
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="AD590">
<pin name="+" direction="in"/>
<pin name="-" direction="in"/>
<pin name="CAN" direction="pas"/>
</symbol>
<symbol name="LM399">
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
</symbol>
<symbol name="565">
<pin name="IN1" direction="in"/>
<pin name="CT" direction="pas"/>
<pin name="IN2" direction="in"/>
<pin name="CV" direction="in"/>
<pin name="RT" direction="pas"/>
<pin name="VCO_IN" direction="in"/>
<pin name="VCO_OUT" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="567">
<pin name="LFIL" direction="pas"/>
<pin name="Q" direction="out"/>
<pin name="CT" direction="pas"/>
<pin name="RT" direction="pas"/>
<pin name="OFIL" direction="out"/>
<pin name="IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AD534">
<pin name="X1" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="SF" direction="in"/>
<pin name="Y1" direction="in"/>
<pin name="Z2" direction="in"/>
<pin name="Z1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="Y2" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="SWSPSTIN">
<pin name="D"/>
<pin name="IN" direction="in" function="dot"/>
<pin name="S"/>
</symbol>
<symbol name="SWSPSTNI">
<pin name="D"/>
<pin name="IN" direction="in"/>
<pin name="S"/>
</symbol>
<symbol name="SWDPST">
<pin name="D1"/>
<pin name="IN" direction="in"/>
<pin name="S1"/>
<pin name="D2"/>
<pin name="S2"/>
</symbol>
<symbol name="PWR+-GSS">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="VL_PIN">
<pin name="VL" direction="in"/>
</symbol>
<symbol name="AD532">
<pin name="X1" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="ON" direction="in"/>
<pin name="Y1" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="Z" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="Y2" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="WR_PIN">
<pin name="!WR" direction="in"/>
</symbol>
<symbol name="SWSPDT">
<pin name="D"/>
<pin name="IN" direction="in"/>
<pin name="S1"/>
<pin name="S2"/>
</symbol>
<symbol name="DG425">
<pin name="IN1" direction="in"/>
<pin name="D1"/>
<pin name="VL" direction="in"/>
<pin name="S1"/>
<pin name="IN2" direction="in"/>
<pin name="!RS" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="D2"/>
<pin name="S2"/>
<pin name="D3"/>
<pin name="S3"/>
<pin name="D4"/>
<pin name="S4"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DG528">
<pin name="D" direction="in"/>
<pin name="S8" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="S1" direction="out"/>
<pin name="EN" direction="in"/>
<pin name="!RS" direction="in" function="dot"/>
<pin name="!WR" direction="in" function="dot"/>
<pin name="S6" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="S5" direction="out"/>
<pin name="S3" direction="out"/>
<pin name="S7" direction="out"/>
<pin name="S4" direction="out"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SD5000">
<pin name="S" direction="in"/>
<pin name="D" direction="out"/>
<pin name="G" direction="in"/>
</symbol>
<symbol name="SD5000/B">
<pin name="B" direction="pwr"/>
</symbol>
<symbol name="NE5205">
<pin name="VCC@2" direction="in"/>
<pin name="VCC@1" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="GND@3" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND@4" direction="in"/>
</symbol>
<symbol name="REF02">
<pin name="OPT" direction="out"/>
<pin name="VO" direction="out"/>
<pin name="TRM" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LM311">
<pin name="ON/STR" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="ON" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="2005">
<pin name="BTSP" direction="pas"/>
<pin name="SVRR" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DAC08">
<pin name="VLC" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="IO" direction="out"/>
<pin name="D1" direction="in"/>
<pin name="!IO" direction="out"/>
<pin name="-VR" direction="in"/>
<pin name="+VR" direction="in"/>
<pin name="CMP" direction="pas"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="LM3914">
<pin name="RHI" direction="in"/>
<pin name="L10" direction="out"/>
<pin name="ADJ" direction="in"/>
<pin name="L9" direction="out"/>
<pin name="VR" direction="out"/>
<pin name="MDE" direction="in"/>
<pin name="RLO" direction="in"/>
<pin name="SIG" direction="in"/>
<pin name="L8" direction="out"/>
<pin name="L7" direction="out"/>
<pin name="L6" direction="out"/>
<pin name="L5" direction="out"/>
<pin name="L4" direction="out"/>
<pin name="L3" direction="out"/>
<pin name="L2" direction="out"/>
<pin name="L1" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="NE5539">
<pin name="CMP" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="ON/AV" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="NE592N8">
<pin name="G1A" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT1" direction="out"/>
<pin name="G1B" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="NPN-L">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="NPN-R">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="MC1648">
<pin name="Q" direction="out"/>
<pin name="TNK" direction="in"/>
<pin name="AGC" direction="pas"/>
<pin name="BS" direction="in"/>
<pin name="V1+" direction="in"/>
<pin name="V2+" direction="in"/>
<pin name="V1-" direction="in"/>
<pin name="V2-" direction="in"/>
</symbol>
<symbol name="LM1871">
<pin name="CH2" direction="out"/>
<pin name="CH4" direction="out"/>
<pin name="MQ" direction="out"/>
<pin name="CH3" direction="out"/>
<pin name="CH1" direction="out"/>
<pin name="CH5" direction="out"/>
<pin name="CH6" direction="out"/>
<pin name="MF" direction="in"/>
<pin name="RFQ" direction="out"/>
<pin name="BS" direction="in"/>
<pin name="PLS" direction="in"/>
<pin name="FRM" direction="in"/>
<pin name="REF" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="RM" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LM1872">
<pin name="XTL" direction="in"/>
<pin name="MXI" direction="in"/>
<pin name="Q1" direction="out"/>
<pin name="VBS" direction="in"/>
<pin name="LO" direction="in"/>
<pin name="MXQ" direction="out"/>
<pin name="IFI" direction="in"/>
<pin name="Q2" direction="out"/>
<pin name="QCA" direction="out"/>
<pin name="QEA" direction="out"/>
<pin name="QCB" direction="out"/>
<pin name="QEB" direction="out"/>
<pin name="GND@1" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="AGC" direction="pas"/>
<pin name="IFQ" direction="out"/>
</symbol>
<symbol name="723">
<pin name="V+" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="+IN" direction="in"/>
<pin name="V-" direction="in"/>
<pin name="VZ" direction="out"/>
<pin name="CL" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="CMP" direction="pas"/>
</symbol>
<symbol name="PWRN">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="2PWRGND">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="ADC0801">
<pin name="CS" direction="in" function="dot"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="INTR" direction="out" function="dot"/>
<pin name="VI+" direction="in"/>
<pin name="VI-" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="DB7" direction="out"/>
<pin name="DB6" direction="out"/>
<pin name="DB5" direction="out"/>
<pin name="DB4" direction="out"/>
<pin name="DB3" direction="out"/>
<pin name="DB2" direction="out"/>
<pin name="DB1" direction="out"/>
<pin name="DB0" direction="out"/>
<pin name="CLKR" direction="in"/>
</symbol>
<symbol name="ADC0808">
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="START" direction="in"/>
<pin name="EOC" direction="out"/>
<pin name="D3" direction="hiz"/>
<pin name="OE" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="VREF+" direction="in"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="VREF-" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="ALE" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
</symbol>
<symbol name="DAC0800">
<pin name="VLC" direction="in"/>
<pin name="!IOUT" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="B8" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="+V" direction="pwr"/>
<pin name="-V" direction="pwr"/>
</symbol>
<symbol name="DAC0808">
<pin name="IOUT" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="COMP" direction="in"/>
</symbol>
<symbol name="ADC0811">
<pin name="VREF" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="D0" direction="out"/>
<pin name="PHI2CLK" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="CH9" direction="in"/>
<pin name="CH8" direction="in"/>
<pin name="CH10" direction="in"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="SCLK" direction="in"/>
<pin name="D1" direction="in"/>
</symbol>
<symbol name="DAC700">
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="B8" direction="in"/>
<pin name="B9" direction="in"/>
<pin name="B10" direction="in"/>
<pin name="B11" direction="in"/>
<pin name="B12" direction="in"/>
<pin name="B13" direction="in"/>
<pin name="B14" direction="in"/>
<pin name="B15" direction="in"/>
<pin name="B16" direction="in"/>
<pin name="RFEEDBCK" direction="out"/>
<pin name="IOUT" direction="out"/>
<pin name="GAINADJ" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="+VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="DAC701">
<pin name="B1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B4" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="B8" direction="in"/>
<pin name="B9" direction="in"/>
<pin name="B10" direction="in"/>
<pin name="B11" direction="in"/>
<pin name="B12" direction="in"/>
<pin name="B13" direction="in"/>
<pin name="B14" direction="in"/>
<pin name="B15" direction="in"/>
<pin name="B16" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="ZEROADJ" direction="out"/>
<pin name="GAINADJ" direction="out"/>
<pin name="REFOUT" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="-VCC" direction="pwr"/>
<pin name="+VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SDM862">
<pin name="MUX_ADD2" direction="in"/>
<pin name="MUX_ADD1" direction="in"/>
<pin name="MUX_ADD0" direction="in"/>
<pin name="MUX_ENA" direction="in"/>
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="S/H_IN" direction="in"/>
<pin name="NC1" direction="nc"/>
<pin name="S/H_O@1" direction="out"/>
<pin name="HOLD_CAP" direction="pas"/>
<pin name="S/H_O@2" direction="out"/>
<pin name="MUX_ADD3" direction="in"/>
<pin name="DCOM(1)" direction="pwr"/>
<pin name="CH8" direction="in"/>
<pin name="CH9" direction="in"/>
<pin name="CH10" direction="in"/>
<pin name="CH11" direction="in"/>
<pin name="CH12" direction="in"/>
<pin name="CH13" direction="in"/>
<pin name="CH14" direction="in"/>
<pin name="CH15" direction="in"/>
<pin name="RG" direction="pas"/>
<pin name="G10" direction="pas"/>
<pin name="G100" direction="pas"/>
<pin name="MO+/AMP+"/>
<pin name="AMP_IN-" direction="in"/>
<pin name="NC2" direction="nc"/>
<pin name="AMP_SENS" direction="out"/>
<pin name="AMP_OUT" direction="out"/>
<pin name="AMP_REF" direction="in"/>
<pin name="+15(1)" direction="pwr"/>
<pin name="-15(1)" direction="pwr"/>
<pin name="+5V(2)" direction="pwr"/>
<pin name="STATUS" direction="out"/>
<pin name="D11" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="S/H_COM2"/>
<pin name="S/H_CONT" direction="in"/>
<pin name="BYTE_SEL" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="DATA_MOD" direction="in"/>
<pin name="R/!C" direction="in"/>
<pin name="CE" direction="in"/>
<pin name="+15(2)" direction="pwr"/>
<pin name="REF_OUT" direction="out"/>
<pin name="ACOM(2)" direction="pwr"/>
<pin name="REF_IN" direction="in"/>
<pin name="BIP_OFF" direction="in"/>
<pin name="ADCIN_10" direction="in"/>
<pin name="ADCIN_20" direction="in"/>
<pin name="-15(2)" direction="pwr"/>
<pin name="DCOM(2)" direction="pwr"/>
<pin name="D0" direction="hiz"/>
</symbol>
<symbol name="AD524">
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="RG1" direction="pas"/>
<pin name="RG2" direction="pas"/>
<pin name="10" direction="out"/>
<pin name="100" direction="out"/>
<pin name="1000" direction="out"/>
<pin name="REF" direction="in"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="SENS" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="O-N2" direction="in"/>
<pin name="O-N1" direction="in"/>
<pin name="I-N2" direction="in"/>
<pin name="I-N1" direction="in"/>
</symbol>
<symbol name="OPAMP+-">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="556">
<pin name="TR" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="R" direction="in" function="dot"/>
<pin name="CV" direction="in"/>
<pin name="THR" direction="in"/>
<pin name="DIS" direction="in"/>
</symbol>
<symbol name="OPAMP+GN">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="2005A">
<pin name="BTSP" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PNP-L">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP-R">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="SSM2402">
<pin name="CTL" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="NC_PIN">
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="PWR+-GR">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LM6325">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V-" direction="pwr"/>
<pin name="V+" direction="pwr"/>
<pin name="FLG"/>
<pin name="S/D"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="V-">
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="AD22050">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="A1" direction="out"/>
<pin name="+VS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OFS" direction="pas"/>
<pin name="A2" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="LM2596">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="LM2596-5">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="EN" direction="in"/>
</symbol>
<symbol name="LM78LXX">
<pin name="VIN" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="LF198">
<pin name="IN" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="!SH" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="LOGREF" direction="pwr"/>
<pin name="OFFSET" direction="in"/>
<pin name="CHOLD" direction="pas"/>
</symbol>
<symbol name="ADC08031">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="VREF" direction="in"/>
<pin name="VIN+" direction="in"/>
<pin name="VIN-" direction="in"/>
</symbol>
<symbol name="ADC08038">
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="CH4" direction="in"/>
<pin name="CH5" direction="in"/>
<pin name="CH6" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="VREF_O" direction="out"/>
<pin name="VREF_I" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="CH7" direction="in"/>
<pin name="COM" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="CLK" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="SE" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="SARS" direction="out"/>
</symbol>
<symbol name="ADC08034">
<pin name="CH0" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH2" direction="in"/>
<pin name="CH3" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="VREF_O" direction="out"/>
<pin name="VREF_I" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="DI" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="CLK" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="SARS" direction="out"/>
</symbol>
<symbol name="ADC08032">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="DI" direction="in"/>
<pin name="CH1" direction="in"/>
<pin name="CH0" direction="in"/>
</symbol>
<symbol name="TDA8501">
<pin name="-(R-Y)" direction="in"/>
<pin name="MCONTROL" direction="in"/>
<pin name="-(B-Y)" direction="in"/>
<pin name="H/2" direction="in"/>
<pin name="Y" direction="in"/>
<pin name="UOFFSET" direction="pas"/>
<pin name="RED" direction="in"/>
<pin name="GREEN" direction="in"/>
<pin name="BLUE" direction="in"/>
<pin name="VOFFSET" direction="pas"/>
<pin name="VREF" direction="pas"/>
<pin name="CHROMA" direction="out"/>
<pin name="FLT" direction="pas"/>
<pin name="CVBS" direction="out"/>
<pin name="PAL/NTSC-Y/Y+SYNC" direction="pas"/>
<pin name="NOTCH" direction="pas"/>
<pin name="Y+SYNCOUT2V" direction="out"/>
<pin name="Y+SYNCIN" direction="in"/>
<pin name="BURSTADJ" direction="pas"/>
<pin name="Y+SYNCOUT1V" direction="out"/>
<pin name="OSC" direction="pas"/>
<pin name="CS" direction="in"/>
</symbol>
<symbol name="SAA1101">
<pin name="FSI" direction="in"/>
<pin name="FSO" direction="out"/>
<pin name="CS1" direction="in"/>
<pin name="CS0" direction="in"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="VLE" direction="in"/>
<pin name="PH" direction="hiz"/>
<pin name="LM1" direction="in"/>
<pin name="LM0" direction="in"/>
<pin name="ECS" direction="in"/>
<pin name="RR" direction="in"/>
<pin name="SI" direction="in"/>
<pin name="ID" direction="out"/>
<pin name="BK" direction="out"/>
<pin name="CB" direction="out"/>
<pin name="CS" direction="out"/>
<pin name="CLP" direction="out"/>
<pin name="WMP" direction="pas"/>
<pin name="VD" direction="out"/>
<pin name="HD" direction="out"/>
<pin name="NORM" direction="in"/>
<pin name="CLO" direction="out"/>
<pin name="X" direction="in"/>
<pin name="Y" direction="in"/>
<pin name="Z" direction="in"/>
</symbol>
<symbol name="VDDVSS">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="VCCVSS">
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MC34119">
<pin name="CD" direction="pas"/>
<pin name="FC1" direction="pas"/>
<pin name="FC2" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VO1" direction="out"/>
<pin name="VO2" direction="out"/>
</symbol>
<symbol name="LM331">
<pin name="I-OUT" direction="out"/>
<pin name="I-REF" direction="pas"/>
<pin name="F-OUT" direction="oc"/>
<pin name="GND" direction="pwr"/>
<pin name="RC" direction="pas"/>
<pin name="THR" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TDA1562">
<pin name="VP1" direction="pwr"/>
<pin name="VP2" direction="pwr"/>
<pin name="PGND1" direction="pwr"/>
<pin name="PGND2" direction="pwr"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="STATUS_IO" direction="in"/>
<pin name="M-SEL" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="SIG-GND" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="OUT+" direction="out"/>
<pin name="OUT-" direction="out"/>
<pin name="DIAGNOSTIC" direction="out"/>
</symbol>
<symbol name="TDA1560Q">
<pin name="VP" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="C1+" direction="pas"/>
<pin name="C1-" direction="pas"/>
<pin name="C2+" direction="pas"/>
<pin name="C2-" direction="pas"/>
<pin name="S1" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="SIG-GND" direction="in"/>
<pin name="INPP" direction="in"/>
<pin name="INPN" direction="in"/>
<pin name="OUT2P" direction="out"/>
<pin name="OUT1N" direction="out"/>
<pin name="VDIAG" direction="out"/>
<pin name="CDEC" direction="pas"/>
<pin name="MODE" direction="in"/>
</symbol>
<symbol name="COMPARATOR-OC">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="oc"/>
</symbol>
<symbol name="TL494">
<pin name="+I1" direction="in"/>
<pin name="+I2" direction="in"/>
<pin name="-I1" direction="in"/>
<pin name="-I2" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="CT" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="E1" direction="pas"/>
<pin name="E2" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUTC" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="DTC" direction="in"/>
</symbol>
<symbol name="TDA1516">
<pin name="VREF" direction="pas"/>
<pin name="IN1-" direction="in"/>
<pin name="IN1+" direction="in"/>
<pin name="IN2+" direction="in"/>
<pin name="STDBY" direction="in"/>
<pin name="INT_VP1/2" direction="pas"/>
<pin name="VP1" direction="pwr"/>
<pin name="VP2" direction="pwr"/>
<pin name="GNDS" direction="pwr"/>
<pin name="GNDP" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="VP" direction="in"/>
</symbol>
<symbol name="ACS">
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="R" direction="pas"/>
</symbol>
<symbol name="LM334-2">
<pin name="V+" direction="pas"/>
<pin name="V-" direction="pas"/>
<pin name="R" direction="pas"/>
<pin name="V-@1" direction="pas"/>
<pin name="V-@2" direction="pas"/>
<pin name="V-@3" direction="pas"/>
</symbol>
<symbol name="MC33215">
<pin name="SLB" direction="in"/>
<pin name="REG" direction="in"/>
<pin name="SLP" direction="in"/>
<pin name="MFI" direction="in"/>
<pin name="HM1" direction="in"/>
<pin name="HM2" direction="in"/>
<pin name="BM2" direction="in"/>
<pin name="BM1" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="TSA" direction="in"/>
<pin name="TSE" direction="in"/>
<pin name="TBN" direction="in"/>
<pin name="!MUT" direction="in"/>
<pin name="NC@1" direction="in"/>
<pin name="NC@2" direction="in"/>
<pin name="SPS" direction="in"/>
<pin name="!PRS" direction="in"/>
<pin name="SWT" direction="in"/>
<pin name="!LSM" direction="in"/>
<pin name="NC@3" direction="in"/>
<pin name="RXS" direction="in"/>
<pin name="RXO" direction="in"/>
<pin name="GRX" direction="in"/>
<pin name="RXI" direction="in"/>
<pin name="NC@4" direction="in"/>
<pin name="NC@5" direction="in"/>
<pin name="RBN" direction="in"/>
<pin name="RSE" direction="in"/>
<pin name="RSA" direction="in"/>
<pin name="RLS" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="AGC" direction="in"/>
<pin name="REF" direction="in"/>
<pin name="SWD" direction="in"/>
<pin name="VOL" direction="in"/>
<pin name="LSI" direction="in"/>
<pin name="PPL" direction="in"/>
<pin name="BVO" direction="in"/>
<pin name="LSF" direction="in"/>
<pin name="NC@6" direction="in"/>
<pin name="NC@7" direction="in"/>
<pin name="LSB" direction="in"/>
<pin name="VLS" direction="in"/>
<pin name="LSO" direction="in"/>
<pin name="PGD" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="VLN" direction="in"/>
<pin name="VHF" direction="in"/>
<pin name="VMC" direction="in"/>
<pin name="NC@8" direction="in"/>
<pin name="NC@9" direction="in"/>
<pin name="NC@10" direction="in"/>
</symbol>
<symbol name="SLA706">
<pin name="OUTA" direction="out"/>
<pin name="OUTA@1" direction="pas"/>
<pin name="SENSEA" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CW/CCW" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="M2" direction="in"/>
<pin name="M1" direction="in"/>
<pin name="M0" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="VBB" direction="pwr"/>
<pin name="SENSEB" direction="in"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTB@1" direction="pas"/>
<pin name="!OUTB" direction="out"/>
<pin name="!OUTB@1" direction="pas"/>
<pin name="!OUTA" direction="out"/>
<pin name="!OUTA@1" direction="pas"/>
</symbol>
<symbol name="LM9044">
<pin name="+" direction="in"/>
<pin name="-" direction="in"/>
<pin name="VREF" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="RF" direction="pas"/>
</symbol>
<symbol name="OPAMP+">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="-V">
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP-OFF+V">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="NULL2" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="NULL1" direction="pas"/>
<pin name="V+" direction="pwr"/>
</symbol>
<symbol name="-V1">
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="TDF8704">
<pin name="VCCA" direction="in"/>
<pin name="O/UF" direction="out"/>
<pin name="VI" direction="in"/>
<pin name="VRB" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="VRT" direction="in"/>
<pin name="D7" direction="out"/>
<pin name="D6" direction="out"/>
<pin name="D5" direction="out"/>
<pin name="D4" direction="out"/>
<pin name="D3" direction="out"/>
<pin name="D2" direction="out"/>
<pin name="D1" direction="out"/>
<pin name="D0" direction="out"/>
<pin name="DEC" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="VCCO1" direction="in"/>
<pin name="VCCO2" direction="in"/>
<pin name="OGND" direction="in"/>
<pin name="DGND" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="VCCD" direction="in"/>
</symbol>
<symbol name="VREG-O4">
<pin name="GND/ADJ" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="OUT@1" direction="pas"/>
<pin name="OUT@2" direction="pas"/>
<pin name="OUT@3" direction="pas"/>
</symbol>
<symbol name="VREG-O2">
<pin name="GND/ADJ" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="OUT@1" direction="pas"/>
</symbol>
<symbol name="TA8210">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="NF1" direction="in"/>
<pin name="NF2" direction="in"/>
<pin name="MUTE_SW" direction="in"/>
<pin name="RIPPLE" direction="in"/>
<pin name="PRE-VCC" direction="pwr"/>
<pin name="PRE-GND" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="STAND-BY_SW" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT3" direction="out"/>
<pin name="OUT4" direction="out"/>
</symbol>
<symbol name="AN7161">
<pin name="HEADPHONE" direction="in"/>
<pin name="RIPPLE" direction="in"/>
<pin name="OUT1A" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="OUT2A" direction="in"/>
<pin name="GND@OUT" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="IN-A" direction="pas"/>
<pin name="IN-B" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="IN" direction="in"/>
</symbol>
<symbol name="LM340S">
<pin name="GND@1" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="PA85">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RCL" direction="in"/>
<pin name="CC" direction="in"/>
<pin name="RC" direction="in"/>
</symbol>
<symbol name="PA241">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="ILIM" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
</symbol>
<symbol name="SA612A">
<pin name="IN-A" direction="in"/>
<pin name="IN-B" direction="in"/>
<pin name="OUT-A" direction="in"/>
<pin name="OUT-B" direction="in"/>
<pin name="OSC'" direction="pas"/>
<pin name="OSC" direction="pas"/>
</symbol>
<symbol name="VCCGND">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="SLA7052">
<pin name="OUTA" direction="out"/>
<pin name="SENSEA" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="FULL/HALF" direction="in"/>
<pin name="CW/CCW" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GATEB" direction="in"/>
<pin name="GATEA" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="VBB" direction="pwr"/>
<pin name="SENSEB" direction="in"/>
<pin name="OUTB" direction="out"/>
<pin name="!OUTB" direction="out"/>
<pin name="!OUTA" direction="out"/>
</symbol>
<symbol name="LM2574">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="pas"/>
<pin name="GND@PWR" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="!ON/OFF" direction="in"/>
<pin name="GNDSIG" direction="in"/>
</symbol>
<symbol name="ERA-3SM">
<pin name="GND@1" direction="pwr"/>
<pin name="RFIN" direction="in"/>
<pin name="RFOUT/DCIN" direction="out"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="MC14536">
<pin name="RESET" direction="in"/>
<pin name="SET" direction="in"/>
<pin name="8-BYPASS" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="OSC-INH" direction="in"/>
<pin name="CLOCK-INH" direction="in"/>
<pin name="MONO-IN" direction="in"/>
<pin name="DECODE" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="RF600T">
<pin name="RXR" direction="in"/>
<pin name="!CTS!/!LOOP" direction="in"/>
<pin name="LEARN/LED"/>
<pin name="!RTS" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="TXH" direction="in"/>
<pin name="RXH" direction="out"/>
<pin name="TXR/HB"/>
<pin name="!TXEN!/RB"/>
<pin name="!RXEN" direction="out"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="OSC1" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="VCC" direction="in"/>
</symbol>
<symbol name="MC1408">
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="COMPEN" direction="pas"/>
<pin name="IO"/>
</symbol>
<symbol name="UDN2954W">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="K" direction="in"/>
<pin name="VREF/!BREAK" direction="in"/>
<pin name="RC" direction="in"/>
<pin name="PHASE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="SENSE" direction="in"/>
<pin name="VBB" direction="pwr"/>
</symbol>
<symbol name="UDN2953B">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="A" direction="in"/>
<pin name="K" direction="in"/>
<pin name="VREF/!BREAK" direction="in"/>
<pin name="RC" direction="in"/>
<pin name="PHASE" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="SENSE" direction="in"/>
<pin name="VBB" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="A3977">
<pin name="OUT1A" direction="out"/>
<pin name="SENSE1" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VBB1" direction="pwr"/>
<pin name="SENSE2" direction="in"/>
<pin name="OUT2B" direction="out"/>
<pin name="OUT2A" direction="out"/>
<pin name="OUT1B" direction="out"/>
<pin name="RC1" direction="pas"/>
<pin name="VREG" direction="pwr"/>
<pin name="CP1" direction="pas"/>
<pin name="CP2" direction="pas"/>
<pin name="STEP" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="HOME" direction="in"/>
<pin name="!SLEEP" direction="in"/>
<pin name="SR" direction="in"/>
<pin name="!ENABLE" direction="in"/>
<pin name="PFD" direction="in"/>
<pin name="RC2" direction="pas"/>
<pin name="VBB2" direction="pwr"/>
<pin name="VCP" direction="pas"/>
</symbol>
<symbol name="A3977PWR">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
</symbol>
<symbol name="A3979">
<pin name="OUT1A" direction="out"/>
<pin name="SENSE1" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="VBB1" direction="pwr"/>
<pin name="SENSE2" direction="in"/>
<pin name="OUT2B" direction="out"/>
<pin name="OUT2A" direction="out"/>
<pin name="OUT1B" direction="out"/>
<pin name="RC1" direction="pas"/>
<pin name="VREG" direction="pwr"/>
<pin name="CP1" direction="pas"/>
<pin name="CP2" direction="pas"/>
<pin name="STEP" direction="in"/>
<pin name="DIR" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="MS1" direction="in"/>
<pin name="MS2" direction="in"/>
<pin name="HOME" direction="in"/>
<pin name="!SLEEP" direction="in"/>
<pin name="SR" direction="in"/>
<pin name="!ENABLE" direction="in"/>
<pin name="PFD" direction="in"/>
<pin name="RC2" direction="pas"/>
<pin name="VBB2" direction="pwr"/>
<pin name="VCP" direction="pas"/>
<pin name="AGND" direction="pwr"/>
<pin name="EXP" direction="pwr"/>
</symbol>
<symbol name="U2400B">
<pin name="+VS" direction="pwr"/>
<pin name="VREF" direction="in"/>
<pin name="VMAX" direction="in"/>
<pin name="VMIN" direction="in"/>
<pin name="TEMP" direction="in"/>
<pin name="PWM" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="STATUS" direction="out"/>
<pin name="DISCHARGE" direction="out"/>
<pin name="TIME" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="0.5HZ"/>
<pin name="FAILURE" direction="in"/>
<pin name="CHARGE" direction="out"/>
</symbol>
<symbol name="LM4995">
<pin name="IN+" direction="in"/>
<pin name="IN-" direction="in"/>
<pin name="!SHDOWN" direction="in"/>
<pin name="BYPASS" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VOL1-" direction="out"/>
<pin name="VOL2+" direction="out"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="MC33164">
<pin name="IN" direction="in"/>
<pin name="!RESET" direction="oc"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="OP+OFFSET">
<pin name="OFF2" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OFF1" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="LM3485">
<pin name="ISENSE" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="PGATE" direction="out"/>
<pin name="FB" direction="in"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="LP3963">
<pin name="VOUT" direction="in"/>
<pin name="!SD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="!ERROR" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="LP3966-ADJ">
<pin name="VOUT" direction="in"/>
<pin name="!SD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="LP3966-SENSE">
<pin name="VOUT" direction="in"/>
<pin name="!SD" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="LT1166">
<pin name="VIN" direction="in"/>
<pin name="VTOP" direction="in"/>
<pin name="VBOTTOM" direction="in"/>
<pin name="SENSE+" direction="in"/>
<pin name="SENSE-" direction="in"/>
<pin name="ILIM+" direction="in"/>
<pin name="ILIM-" direction="in"/>
<pin name="VOUT" direction="out"/>
</symbol>
<symbol name="TL770X">
<pin name="+VS" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="!RESIN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="RESET" direction="oc"/>
<pin name="!RESET" direction="oc"/>
<pin name="REF" direction="in"/>
</symbol>
<symbol name="PWR-VDDGND">
<pin name="VDD" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LM317LD">
<pin name="VI" direction="in"/>
<pin name="ADJ" direction="in"/>
<pin name="VO" direction="pas"/>
<pin name="VO@1" direction="pas"/>
<pin name="VO@2" direction="pas"/>
<pin name="VO@3" direction="pas"/>
</symbol>
<symbol name="LM3524">
<pin name="VIN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="COMP" direction="in"/>
<pin name="+CLSENSE" direction="in"/>
<pin name="-CLSENSE" direction="in"/>
<pin name="SHUTDOWN" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OSCOUT" direction="out"/>
<pin name="VREF" direction="pas"/>
<pin name="CA" direction="pas"/>
<pin name="EA" direction="pas"/>
<pin name="CB" direction="pas"/>
<pin name="EB" direction="pas"/>
</symbol>
<symbol name="LM3525-L">
<pin name="IN" direction="in"/>
<pin name="FLAG" direction="out"/>
<pin name="!EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="LM3525-H">
<pin name="IN" direction="in"/>
<pin name="FLAG" direction="out"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="OUT@1" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="AMP_GND_GAIN_BYP">
<pin name="GAIN@1" direction="pas"/>
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="GAIN@2" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VS" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="BYPASS" direction="pas"/>
</symbol>
<symbol name="78XX2GND">
<pin name="VI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="pas"/>
<pin name="GND@1" direction="pas"/>
</symbol>
<symbol name="PA02">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT@2" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="RCL+" direction="in"/>
<pin name="RCL-" direction="in"/>
<pin name="OUT@1" direction="out"/>
</symbol>
<symbol name="GVA-84">
<pin name="GND@1" direction="pwr"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="MC34025">
<pin name="VREF" direction="in"/>
<pin name="CLOCK" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="RAMP" direction="in"/>
<pin name="ERROR" direction="out"/>
<pin name="+IN" direction="in"/>
<pin name="-IN" direction="in"/>
<pin name="SOFT-START" direction="in"/>
<pin name="LIM/SH-DOWN" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
</symbol>
<symbol name="LM5030">
<pin name="VIN" direction="in"/>
<pin name="VFB" direction="in"/>
<pin name="COMP" direction="out"/>
<pin name="SS" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CS" direction="pas"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LP2950">
<pin name="I" direction="in"/>
<pin name="O" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="LP2951">
<pin name="OUT" direction="in"/>
<pin name="SENSE" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="SH-DOWN" direction="in"/>
<pin name="!ERROR" direction="out"/>
<pin name="VOTAB" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="UUC1806">
<pin name="VIN" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="NI" direction="in"/>
<pin name="CURLIM" direction="in"/>
<pin name="SYNC" direction="in"/>
<pin name="RT" direction="in"/>
<pin name="CS-" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="CS+" direction="in"/>
<pin name="SH-DOWN" direction="in"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTA" direction="out"/>
<pin name="COMP" direction="in"/>
<pin name="INV" direction="in"/>
<pin name="VC" direction="pwr"/>
</symbol>
<symbol name="LM50">
<pin name="+VS" direction="in"/>
<pin name="VO" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="PA94">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="ILIM" direction="in"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
</symbol>
<symbol name="REF102">
<pin name="NOIS" direction="pas"/>
<pin name="VO" direction="out"/>
<pin name="TRM" direction="in"/>
<pin name="V+" direction="in"/>
<pin name="COM" direction="in"/>
</symbol>
<symbol name="INVERTER">
<pin name="I" direction="in"/>
<pin name="O" direction="in"/>
</symbol>
<symbol name="GND">
<pin name="O" direction="in"/>
</symbol>
<symbol name="LM336">
<pin name="A" direction="in"/>
<pin name="C" direction="pas"/>
<pin name="ADJ" direction="in"/>
</symbol>
<symbol name="OPAMP+-CS">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="!CS" direction="in"/>
</symbol>
<symbol name="MC1350">
<pin name="IN-" direction="in"/>
<pin name="IN+" direction="in"/>
<pin name="AGC" direction="in"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT+" direction="in"/>
<pin name="OUT-" direction="in"/>
<pin name="45/58MHZ" direction="pas"/>
</symbol>
<symbol name="TA7358P">
<pin name="RF-IN" direction="in"/>
<pin name="RF-OUT" direction="in"/>
<pin name="MIX-IN" direction="in"/>
<pin name="MIX-OUT" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="RF-BY-PASS" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="OSC-MONI" direction="in"/>
</symbol>
<symbol name="MCP1703">
<pin name="VI" direction="in"/>
<pin name="GND" direction="pas"/>
<pin name="VO" direction="pas"/>
<pin name="VI1" direction="in"/>
</symbol>
<symbol name="DAC0808D">
<pin name="IOUT" direction="out"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="VREF+" direction="in"/>
<pin name="VREF-" direction="in"/>
<pin name="COMP" direction="in"/>
</symbol>
<symbol name="OPA726">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="DGND" direction="in"/>
</symbol>
<symbol name="OPA2726">
<pin name="-INA" direction="in"/>
<pin name="+INA" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="EN" direction="in"/>
<pin name="-INB" direction="in"/>
<pin name="+INB" direction="in"/>
<pin name="OUTB" direction="out"/>
<pin name="DGND" direction="in"/>
</symbol>
<symbol name="OPAMP-BAL-CMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="BAL2" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="BAL1" direction="pas"/>
<pin name="V+" direction="pwr"/>
<pin name="COMP" direction="pas"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="OPAMP_CS">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="!CS" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="2CMP" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2CMP"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2NUL2CMP" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2NUL_1+5" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2NUL_1+8" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="1AMP_P7+4" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2AMP_P8+4" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4AMP_P4+11" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4AMP_P11+7" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="13"/>
<connect gate="D" pin="-IN" pad="14"/>
<connect gate="D" pin="OUT" pad="12"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="13"/>
<connect gate="D" pin="-IN" pad="14"/>
<connect gate="D" pin="OUT" pad="12"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4AMP_P3+12" prefix="IC" uservalue="yes">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP08" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2CMP"/>
</gates>
<devices>
<device name="J" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM308" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2CMP"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LH0044H" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2CMP"/>
</gates>
<devices>
<device name="" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP2" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM201" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM301" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="H" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*748" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="UA"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="UA"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD507" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD509" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CA3130" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="T" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CA3140" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="T" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM318" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/CMP" pad="1"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD504" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD510" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD517" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP07*" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
</technologies>
</device>
<device name="R" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="C"/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="C"/>
<technology name="D"/>
<technology name="E"/>
<technology name="Z"/>
</technologies>
</device>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="CQ"/>
<technology name="DQ"/>
<technology name="EQ"/>
<technology name="Q"/>
<technology name="Z"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP27" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="J" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="Z" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP37" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="Z" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP77" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="J" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="Z" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM101" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD847" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*3080" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD515" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD540" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="H" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*741" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="UA"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="UA"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF355" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF356" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF357" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF351" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF411" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF441" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LH0042H" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL081" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL061" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL071" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD548" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD711" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP90" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP42" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="Z" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA121" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="8"/>
<connect gate="A" pin="OPT" pad="5"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA606" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CA5160E" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC251" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC271" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7611" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM833" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33078" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC272" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7621" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD648" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP200" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD712" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2111" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5532" prefix="IC">
<description>&lt;b&gt;AUDIO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CA3240E" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CA5260E" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM393" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*4558" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC393" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL062" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL072" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM358" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt; also LM158; LM258; LM2904&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM158.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MX" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL082" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;&lt;p&gt;
&lt;a href = "http://www.ti.com/lit/ds/symlink/tl084a . pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA_SHEET" value="&lt;a href=&quot;http://www.ti.com/lit/ds/symlink/tl084a.pdf&quot;&gt; Data sheet &lt;/a&gt;"/>
</technology>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA_SHEET" value="&lt;a href=&quot;http://www.ti.com/lit/ds/symlink/tl084a.pdf&quot;&gt; Data sheet &lt;/a&gt;"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2320A" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF412" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF442" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2903" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF353" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34002" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RC4559" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*1458" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP09" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="13"/>
<connect gate="D" pin="-IN" pad="14"/>
<connect gate="D" pin="OUT" pad="12"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="13"/>
<connect gate="D" pin="-IN" pad="14"/>
<connect gate="D" pin="OUT" pad="12"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RC4156DB" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="13"/>
<connect gate="D" pin="-IN" pad="14"/>
<connect gate="D" pin="OUT" pad="12"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="13"/>
<connect gate="D" pin="-IN" pad="14"/>
<connect gate="D" pin="OUT" pad="12"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP11" prefix="IC">
<description>&lt;b&gt;Quad Low-Offset Low-Power OP AMP&lt;/b&gt;&lt;p&gt;
The OP-11 is pin compatible with the OP-400 , LM148, HA4741, RM4156, and LT1014 operational amplifiers&lt;p&gt;
source  http://products.analog.com/products/info.asp?product=OP400</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="DIL16">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="12"/>
<connect gate="C" pin="-IN" pad="11"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="14"/>
<connect gate="D" pin="-IN" pad="15"/>
<connect gate="D" pin="OUT" pad="16"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="TC" package="PLCC28S">
<connects>
<connect gate="A" pin="+IN" pad="6"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="10"/>
<connect gate="B" pin="-IN" pad="13"/>
<connect gate="B" pin="OUT" pad="14"/>
<connect gate="C" pin="+IN" pad="20"/>
<connect gate="C" pin="-IN" pad="17"/>
<connect gate="C" pin="OUT" pad="16"/>
<connect gate="D" pin="+IN" pad="24"/>
<connect gate="D" pin="-IN" pad="27"/>
<connect gate="D" pin="OUT" pad="28"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL074" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL064" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL084" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA404" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP471" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP470" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP490" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC274" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7641" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ICL7642" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP400" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33079" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RC4136" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="13"/>
<connect gate="D" pin="-IN" pad="14"/>
<connect gate="D" pin="OUT" pad="12"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="10"/>
<connect gate="D" pin="+IN" pad="13"/>
<connect gate="D" pin="-IN" pad="14"/>
<connect gate="D" pin="OUT" pad="12"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM324" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2902" prefix="IC">
<description>&lt;b&gt;Low power quad operational amplifier&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00000533.pdf"&gt; Data sgeet &lt;/a&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PT" package="SSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF347" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34004" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM339" prefix="IC">
<description>&lt;b&gt;Low Power Low Offset Voltage Quad Comparators&lt;/b&gt;&lt;p&gt;
with open collector; LM139/LM239/LM339/LM2901/LM3302&lt;br&gt;</description>
<gates>
<gate name="P" symbol="PWR+G"/>
<gate name="A" symbol="COMPARATOR-OC"/>
<gate name="B" symbol="COMPARATOR-OC"/>
<gate name="C" symbol="COMPARATOR-OC"/>
<gate name="D" symbol="COMPARATOR-OC"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="V+" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC339" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2901" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC3302" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="7"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="1"/>
<connect gate="C" pin="+IN" pad="9"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="11"/>
<connect gate="D" pin="-IN" pad="10"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LH0002N" prefix="IC">
<description>&lt;b&gt;BUFFER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="LH0002"/>
</gates>
<devices>
<device name="" package="DIL10">
<connects>
<connect gate="A" pin="E3" pad="9"/>
<connect gate="A" pin="E4" pad="7"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="V1+" pad="2"/>
<connect gate="A" pin="V1-" pad="4"/>
<connect gate="A" pin="V2+" pad="1"/>
<connect gate="A" pin="V2-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LH0003H" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="LH0004"/>
</gates>
<devices>
<device name="" package="TO100">
<connects>
<connect gate="A" pin="+IN" pad="10"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="BS1" pad="3"/>
<connect gate="A" pin="BS2" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP1/CL" pad="4"/>
<connect gate="A" pin="CMP2" pad="7"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LH0004H" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="LH0004"/>
</gates>
<devices>
<device name="" package="TO100">
<connects>
<connect gate="A" pin="+IN" pad="10"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="BS1" pad="3"/>
<connect gate="A" pin="BS2" pad="2"/>
<connect gate="A" pin="CMP1" pad="1"/>
<connect gate="A" pin="CMP1/CL" pad="4"/>
<connect gate="A" pin="CMP2" pad="7"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*555" prefix="IC">
<description>&lt;b&gt;TIMER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="555"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="CV" pad="5"/>
<connect gate="A" pin="DIS" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="Q" pad="3"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="THR" pad="6"/>
<connect gate="A" pin="TR" pad="2"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="NE"/>
<technology name="SE"/>
<technology name="UA"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="CV" pad="5"/>
<connect gate="A" pin="DIS" pad="7"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="Q" pad="3"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="THR" pad="6"/>
<connect gate="A" pin="TR" pad="2"/>
<connect gate="A" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="NE"/>
<technology name="SE"/>
<technology name="UA"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78*" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;&lt;p&gt;
Source:&lt;br&gt;
http://cache.national.com/ds/LM/LM78L05.pdf&lt;br&gt;
http://www.fairchildsemi.com/ds/LM/LM7805.pdf</description>
<gates>
<gate name="A1" symbol="78XX"/>
</gates>
<devices>
<device name="Z" package="TO92">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="VI" pad="3"/>
<connect gate="A1" pin="VO" pad="1"/>
</connects>
<technologies>
<technology name="L05"/>
<technology name="L08"/>
<technology name="L12"/>
<technology name="L15"/>
<technology name="L18"/>
<technology name="L24"/>
</technologies>
</device>
<device name="T" package="TO220H">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="VI" pad="1"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="H" package="TO39">
<connects>
<connect gate="A1" pin="GND" pad="3"/>
<connect gate="A1" pin="VI" pad="1"/>
<connect gate="A1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="L" package="TO92">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="VI" pad="3"/>
<connect gate="A1" pin="VO" pad="1"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="DT" package="TO252">
<connects>
<connect gate="A1" pin="GND" pad="3"/>
<connect gate="A1" pin="VI" pad="1"/>
<connect gate="A1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="TV" package="TO220V">
<connects>
<connect gate="A1" pin="GND" pad="2"/>
<connect gate="A1" pin="VI" pad="1"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="79*" prefix="IC" uservalue="yes">
<description>Negative &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="A1" symbol="79XX"/>
</gates>
<devices>
<device name="L" package="TO92">
<connects>
<connect gate="A1" pin="GND" pad="1"/>
<connect gate="A1" pin="VI" pad="2"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="H" package="TO39">
<connects>
<connect gate="A1" pin="GND" pad="1"/>
<connect gate="A1" pin="VI" pad="2"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="T" package="TO220H">
<connects>
<connect gate="A1" pin="GND" pad="1"/>
<connect gate="A1" pin="VI" pad="2"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="Z" package="TO92">
<connects>
<connect gate="A1" pin="GND" pad="1"/>
<connect gate="A1" pin="VI" pad="2"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="L05"/>
<technology name="L08"/>
<technology name="L12"/>
<technology name="L15"/>
<technology name="L18"/>
<technology name="L24"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*317" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="A1" symbol="317"/>
</gates>
<devices>
<device name="LZ" package="TO92">
<connects>
<connect gate="A1" pin="ADJ" pad="1"/>
<connect gate="A1" pin="VI" pad="3"/>
<connect gate="A1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
<device name="T" package="TO220H">
<connects>
<connect gate="A1" pin="ADJ" pad="1"/>
<connect gate="A1" pin="VI" pad="3"/>
<connect gate="A1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EMP" package="SOT223">
<connects>
<connect gate="A1" pin="ADJ" pad="1"/>
<connect gate="A1" pin="VI" pad="3"/>
<connect gate="A1" pin="VO" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*337" prefix="IC">
<description>Negative &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="A1" symbol="337"/>
</gates>
<devices>
<device name="LZ" package="TO92">
<connects>
<connect gate="A1" pin="ADJ" pad="1"/>
<connect gate="A1" pin="VI" pad="3"/>
<connect gate="A1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
<device name="T" package="TO220H">
<connects>
<connect gate="A1" pin="ADJ" pad="1"/>
<connect gate="A1" pin="VI" pad="2"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="IMP" package="SOT223">
<connects>
<connect gate="A1" pin="ADJ" pad="1"/>
<connect gate="A1" pin="VI" pad="4"/>
<connect gate="A1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3900" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="LM3900"/>
<gate name="B" symbol="LM3900"/>
<gate name="C" symbol="LM3900"/>
<gate name="D" symbol="LM3900"/>
<gate name="P" symbol="PWR+G"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="6"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="B" pin="+IN" pad="2"/>
<connect gate="B" pin="-IN" pad="3"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="13"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="9"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="11"/>
<connect gate="D" pin="OUT" pad="10"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="V+" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="6"/>
<connect gate="A" pin="OUT" pad="5"/>
<connect gate="B" pin="+IN" pad="2"/>
<connect gate="B" pin="-IN" pad="3"/>
<connect gate="B" pin="OUT" pad="4"/>
<connect gate="C" pin="+IN" pad="13"/>
<connect gate="C" pin="-IN" pad="8"/>
<connect gate="C" pin="OUT" pad="9"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="11"/>
<connect gate="D" pin="OUT" pad="10"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="V+" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD590H" prefix="IC">
<description>&lt;b&gt;TEMPERATURE SENSOR&lt;/b&gt;&lt;p&gt;
current output</description>
<gates>
<gate name="A" symbol="AD590"/>
</gates>
<devices>
<device name="" package="TO18">
<connects>
<connect gate="A" pin="+" pad="1"/>
<connect gate="A" pin="-" pad="2"/>
<connect gate="A" pin="CAN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD590ZR" prefix="IC">
<description>&lt;b&gt;TEMPERATURE SENSOR&lt;/b&gt;&lt;p&gt;
current output</description>
<gates>
<gate name="A" symbol="AD590"/>
</gates>
<devices>
<device name="" package="TO92">
<connects>
<connect gate="A" pin="+" pad="1"/>
<connect gate="A" pin="-" pad="2"/>
<connect gate="A" pin="CAN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM399H" prefix="IC">
<description>Precision &lt;b&gt;Z DIODE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="LM399"/>
</gates>
<devices>
<device name="" package="TO39/4">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
<connect gate="A" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM675T" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="" package="CB367">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1875T" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="" package="CB367">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM383T" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+GN"/>
</gates>
<devices>
<device name="" package="CB367">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM307" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*556" prefix="IC">
<description>Dual &lt;b&gt;TIMER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="555"/>
<gate name="B" symbol="556"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="CV" pad="3"/>
<connect gate="A" pin="DIS" pad="1"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="THR" pad="2"/>
<connect gate="A" pin="TR" pad="6"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="B" pin="CV" pad="11"/>
<connect gate="B" pin="DIS" pad="13"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="B" pin="R" pad="10"/>
<connect gate="B" pin="THR" pad="12"/>
<connect gate="B" pin="TR" pad="8"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="NE"/>
<technology name="SE"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="CV" pad="3"/>
<connect gate="A" pin="DIS" pad="1"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="Q" pad="5"/>
<connect gate="A" pin="R" pad="4"/>
<connect gate="A" pin="THR" pad="2"/>
<connect gate="A" pin="TR" pad="6"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="B" pin="CV" pad="11"/>
<connect gate="B" pin="DIS" pad="13"/>
<connect gate="B" pin="Q" pad="9"/>
<connect gate="B" pin="R" pad="10"/>
<connect gate="B" pin="THR" pad="12"/>
<connect gate="B" pin="TR" pad="8"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="NE"/>
<technology name="SE"/>
<technology name="UA"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*565H" prefix="IC">
<description>&lt;b&gt;PLL&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="565"/>
</gates>
<devices>
<device name="" package="TO100">
<connects>
<connect gate="A" pin="CT" pad="9"/>
<connect gate="A" pin="CV" pad="7"/>
<connect gate="A" pin="IN1" pad="2"/>
<connect gate="A" pin="IN2" pad="3"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="RT" pad="8"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="1"/>
<connect gate="A" pin="VCO_IN" pad="5"/>
<connect gate="A" pin="VCO_OUT" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*567" prefix="IC">
<description>&lt;b&gt;TONE DECODER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="567"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="CT" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="LFIL" pad="2"/>
<connect gate="A" pin="OFIL" pad="1"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="NE"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="CT" pad="6"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="3"/>
<connect gate="A" pin="LFIL" pad="2"/>
<connect gate="A" pin="OFIL" pad="1"/>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="RT" pad="5"/>
<connect gate="A" pin="V+" pad="4"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="NE"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD534H" prefix="IC">
<description>&lt;b&gt;MULTIPLIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="AD534"/>
</gates>
<devices>
<device name="" package="TO100">
<connects>
<connect gate="A" pin="Q" pad="8"/>
<connect gate="A" pin="SF" pad="2"/>
<connect gate="A" pin="V+" pad="9"/>
<connect gate="A" pin="V-" pad="5"/>
<connect gate="A" pin="X1" pad="10"/>
<connect gate="A" pin="X2" pad="1"/>
<connect gate="A" pin="Y1" pad="3"/>
<connect gate="A" pin="Y2" pad="4"/>
<connect gate="A" pin="Z1" pad="7"/>
<connect gate="A" pin="Z2" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD532H" prefix="IC">
<description>&lt;b&gt;MULTIPLIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="AD532"/>
</gates>
<devices>
<device name="" package="TO100">
<connects>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="ON" pad="9"/>
<connect gate="A" pin="Q" pad="4"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
<connect gate="A" pin="X1" pad="6"/>
<connect gate="A" pin="X2" pad="7"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="10"/>
<connect gate="A" pin="Z" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD632H" prefix="IC">
<description>&lt;b&gt;MULTIPLIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="AD532"/>
</gates>
<devices>
<device name="" package="TO100">
<connects>
<connect gate="A" pin="GND" pad="8"/>
<connect gate="A" pin="ON" pad="9"/>
<connect gate="A" pin="Q" pad="4"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="V-" pad="5"/>
<connect gate="A" pin="X1" pad="6"/>
<connect gate="A" pin="X2" pad="7"/>
<connect gate="A" pin="Y1" pad="1"/>
<connect gate="A" pin="Y2" pad="10"/>
<connect gate="A" pin="Z" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3524" prefix="IC">
<description>&lt;b&gt;Regulating Pulse Width Modulator&lt;/b&gt; LM2524D/LM3524D&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM2524D.pdf</description>
<gates>
<gate name="G$1" symbol="LM3524"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="+CLSENSE" pad="4"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-CLSENSE" pad="5"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="CA" pad="12"/>
<connect gate="G$1" pin="CB" pad="13"/>
<connect gate="G$1" pin="COMP" pad="9"/>
<connect gate="G$1" pin="CT" pad="7"/>
<connect gate="G$1" pin="EA" pad="11"/>
<connect gate="G$1" pin="EB" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="OSCOUT" pad="3"/>
<connect gate="G$1" pin="RT" pad="6"/>
<connect gate="G$1" pin="SHUTDOWN" pad="10"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VREF" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="G$1" pin="+CLSENSE" pad="4"/>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-CLSENSE" pad="5"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="CA" pad="12"/>
<connect gate="G$1" pin="CB" pad="13"/>
<connect gate="G$1" pin="COMP" pad="9"/>
<connect gate="G$1" pin="CT" pad="7"/>
<connect gate="G$1" pin="EA" pad="11"/>
<connect gate="G$1" pin="EB" pad="14"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="OSCOUT" pad="3"/>
<connect gate="G$1" pin="RT" pad="6"/>
<connect gate="G$1" pin="SHUTDOWN" pad="10"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VREF" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG201CJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="C" symbol="SWSPSTIN"/>
<gate name="D" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG271CJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="C" symbol="SWSPSTIN"/>
<gate name="D" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG309DJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="C" symbol="SWSPSTIN"/>
<gate name="D" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HI201/5" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="C" symbol="SWSPSTIN"/>
<gate name="D" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG211CJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="C" symbol="SWSPSTIN"/>
<gate name="D" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG221K" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="C" symbol="SWSPSTIN"/>
<gate name="D" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="\WR" symbol="WR_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="\WR" pin="!WR" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="\WR" pin="!WR" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG411CJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="C" symbol="SWSPSTIN"/>
<gate name="D" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG202CJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTNI"/>
<gate name="B" symbol="SWSPSTNI"/>
<gate name="C" symbol="SWSPSTNI"/>
<gate name="D" symbol="SWSPSTNI"/>
<gate name="P" symbol="PWR+-GSS"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG308DJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTNI"/>
<gate name="B" symbol="SWSPSTNI"/>
<gate name="C" symbol="SWSPSTNI"/>
<gate name="D" symbol="SWSPSTNI"/>
<gate name="P" symbol="PWR+-GSS"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG212CJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTNI"/>
<gate name="B" symbol="SWSPSTNI"/>
<gate name="C" symbol="SWSPSTNI"/>
<gate name="D" symbol="SWSPSTNI"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADG222K" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTNI"/>
<gate name="B" symbol="SWSPSTNI"/>
<gate name="C" symbol="SWSPSTNI"/>
<gate name="D" symbol="SWSPSTNI"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="\WR" symbol="WR_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="\WR" pin="!WR" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="\WR" pin="!WR" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG412DJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTNI"/>
<gate name="B" symbol="SWSPSTNI"/>
<gate name="C" symbol="SWSPSTNI"/>
<gate name="D" symbol="SWSPSTNI"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG403DJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWDPST"/>
<gate name="B" symbol="SWDPST"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D1" pad="1"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="IN" pad="15"/>
<connect gate="A" pin="S1" pad="16"/>
<connect gate="A" pin="S2" pad="4"/>
<connect gate="B" pin="D1" pad="8"/>
<connect gate="B" pin="D2" pad="6"/>
<connect gate="B" pin="IN" pad="10"/>
<connect gate="B" pin="S1" pad="9"/>
<connect gate="B" pin="S2" pad="5"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="14"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D1" pad="1"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="IN" pad="15"/>
<connect gate="A" pin="S1" pad="16"/>
<connect gate="A" pin="S2" pad="4"/>
<connect gate="B" pin="D1" pad="8"/>
<connect gate="B" pin="D2" pad="6"/>
<connect gate="B" pin="IN" pad="10"/>
<connect gate="B" pin="S1" pad="9"/>
<connect gate="B" pin="S2" pad="5"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="14"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG5043CJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWDPST"/>
<gate name="B" symbol="SWDPST"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D1" pad="1"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="IN" pad="15"/>
<connect gate="A" pin="S1" pad="16"/>
<connect gate="A" pin="S2" pad="4"/>
<connect gate="B" pin="D1" pad="8"/>
<connect gate="B" pin="D2" pad="6"/>
<connect gate="B" pin="IN" pad="10"/>
<connect gate="B" pin="S1" pad="9"/>
<connect gate="B" pin="S2" pad="5"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="14"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D1" pad="1"/>
<connect gate="A" pin="D2" pad="3"/>
<connect gate="A" pin="IN" pad="15"/>
<connect gate="A" pin="S1" pad="16"/>
<connect gate="A" pin="S2" pad="4"/>
<connect gate="B" pin="D1" pad="8"/>
<connect gate="B" pin="D2" pad="6"/>
<connect gate="B" pin="IN" pad="10"/>
<connect gate="B" pin="S1" pad="9"/>
<connect gate="B" pin="S2" pad="5"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="V+" pad="11"/>
<connect gate="P" pin="V-" pad="14"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG200CJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="IN" pad="14"/>
<connect gate="A" pin="S" pad="10"/>
<connect gate="B" pin="D" pad="6"/>
<connect gate="B" pin="IN" pad="1"/>
<connect gate="B" pin="S" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="12"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="IN" pad="14"/>
<connect gate="A" pin="S" pad="10"/>
<connect gate="B" pin="D" pad="6"/>
<connect gate="B" pin="IN" pad="1"/>
<connect gate="B" pin="S" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="12"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HI200/5" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTIN"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="IN" pad="14"/>
<connect gate="A" pin="S" pad="10"/>
<connect gate="B" pin="D" pad="6"/>
<connect gate="B" pin="IN" pad="1"/>
<connect gate="B" pin="S" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="12"/>
<connect gate="P" pin="V-" pad="7"/>
<connect gate="VL" pin="VL" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="IN" pad="14"/>
<connect gate="A" pin="S" pad="10"/>
<connect gate="B" pin="D" pad="6"/>
<connect gate="B" pin="IN" pad="1"/>
<connect gate="B" pin="S" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="12"/>
<connect gate="P" pin="V-" pad="7"/>
<connect gate="VL" pin="VL" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG413DJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTNI"/>
<gate name="B" symbol="SWSPSTIN"/>
<gate name="C" symbol="SWSPSTIN"/>
<gate name="D" symbol="SWSPSTNI"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="3"/>
<connect gate="B" pin="D" pad="15"/>
<connect gate="B" pin="IN" pad="16"/>
<connect gate="B" pin="S" pad="14"/>
<connect gate="C" pin="D" pad="10"/>
<connect gate="C" pin="IN" pad="9"/>
<connect gate="C" pin="S" pad="11"/>
<connect gate="D" pin="D" pad="7"/>
<connect gate="D" pin="IN" pad="8"/>
<connect gate="D" pin="S" pad="6"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
<connect gate="VL" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG419DJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPDT"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="IN" pad="6"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="8"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="7"/>
<connect gate="VL" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="IN" pad="6"/>
<connect gate="A" pin="S1" pad="2"/>
<connect gate="A" pin="S2" pad="8"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="7"/>
<connect gate="VL" pin="VL" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG425DJ" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="DG425"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!RS" pad="7"/>
<connect gate="A" pin="!WR" pad="2"/>
<connect gate="A" pin="D1" pad="1"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="D3" pad="3"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="IN1" pad="15"/>
<connect gate="A" pin="IN2" pad="10"/>
<connect gate="A" pin="S1" pad="16"/>
<connect gate="A" pin="S2" pad="9"/>
<connect gate="A" pin="S3" pad="4"/>
<connect gate="A" pin="S4" pad="5"/>
<connect gate="A" pin="V+" pad="11"/>
<connect gate="A" pin="V-" pad="14"/>
<connect gate="A" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!RS" pad="7"/>
<connect gate="A" pin="!WR" pad="2"/>
<connect gate="A" pin="D1" pad="1"/>
<connect gate="A" pin="D2" pad="8"/>
<connect gate="A" pin="D3" pad="3"/>
<connect gate="A" pin="D4" pad="6"/>
<connect gate="A" pin="GND" pad="13"/>
<connect gate="A" pin="IN1" pad="15"/>
<connect gate="A" pin="IN2" pad="10"/>
<connect gate="A" pin="S1" pad="16"/>
<connect gate="A" pin="S2" pad="9"/>
<connect gate="A" pin="S3" pad="4"/>
<connect gate="A" pin="S4" pad="5"/>
<connect gate="A" pin="V+" pad="11"/>
<connect gate="A" pin="V-" pad="14"/>
<connect gate="A" pin="VL" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DG528CJ" prefix="IC">
<description>&lt;b&gt;MULTIPLEXER&lt;/b&gt;&lt;p&gt;
latched 4/8-channel analog multiplexer</description>
<gates>
<gate name="A" symbol="DG528"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="A" pin="!RS" pad="18"/>
<connect gate="A" pin="!WR" pad="1"/>
<connect gate="A" pin="A0" pad="2"/>
<connect gate="A" pin="A1" pad="17"/>
<connect gate="A" pin="A2" pad="16"/>
<connect gate="A" pin="D" pad="9"/>
<connect gate="A" pin="EN" pad="3"/>
<connect gate="A" pin="GND" pad="15"/>
<connect gate="A" pin="S1" pad="5"/>
<connect gate="A" pin="S2" pad="6"/>
<connect gate="A" pin="S3" pad="7"/>
<connect gate="A" pin="S4" pad="8"/>
<connect gate="A" pin="S5" pad="13"/>
<connect gate="A" pin="S6" pad="12"/>
<connect gate="A" pin="S7" pad="11"/>
<connect gate="A" pin="S8" pad="10"/>
<connect gate="A" pin="V+" pad="14"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IH5352P" prefix="IC">
<description>&lt;b&gt;CMOS SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SWSPSTNI"/>
<gate name="B" symbol="SWSPSTNI"/>
<gate name="C" symbol="SWSPSTNI"/>
<gate name="D" symbol="SWSPSTNI"/>
<gate name="P" symbol="PWR+-GSS"/>
<gate name="VL" symbol="VL_PIN"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="16"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
<connect gate="B" pin="D" pad="14"/>
<connect gate="B" pin="IN" pad="3"/>
<connect gate="B" pin="S" pad="4"/>
<connect gate="C" pin="D" pad="12"/>
<connect gate="C" pin="IN" pad="5"/>
<connect gate="C" pin="S" pad="6"/>
<connect gate="D" pin="D" pad="10"/>
<connect gate="D" pin="IN" pad="7"/>
<connect gate="D" pin="S" pad="8"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="V+" pad="15"/>
<connect gate="P" pin="V-" pad="11"/>
<connect gate="VL" pin="VL" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="16"/>
<connect gate="A" pin="IN" pad="1"/>
<connect gate="A" pin="S" pad="2"/>
<connect gate="B" pin="D" pad="14"/>
<connect gate="B" pin="IN" pad="3"/>
<connect gate="B" pin="S" pad="4"/>
<connect gate="C" pin="D" pad="12"/>
<connect gate="C" pin="IN" pad="5"/>
<connect gate="C" pin="S" pad="6"/>
<connect gate="D" pin="D" pad="10"/>
<connect gate="D" pin="IN" pad="7"/>
<connect gate="D" pin="S" pad="8"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="V+" pad="15"/>
<connect gate="P" pin="V-" pad="11"/>
<connect gate="VL" pin="VL" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SD5000" prefix="IC">
<description>DMOS &lt;b&gt;SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SD5000"/>
<gate name="P" symbol="SD5000/B"/>
<gate name="B" symbol="SD5000"/>
<gate name="C" symbol="SD5000"/>
<gate name="D" symbol="SD5000"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="4"/>
<connect gate="B" pin="D" pad="8"/>
<connect gate="B" pin="G" pad="6"/>
<connect gate="B" pin="S" pad="5"/>
<connect gate="C" pin="D" pad="9"/>
<connect gate="C" pin="G" pad="11"/>
<connect gate="C" pin="S" pad="12"/>
<connect gate="D" pin="D" pad="16"/>
<connect gate="D" pin="G" pad="14"/>
<connect gate="D" pin="S" pad="13"/>
<connect gate="P" pin="B" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="D" pad="1"/>
<connect gate="A" pin="G" pad="3"/>
<connect gate="A" pin="S" pad="4"/>
<connect gate="B" pin="D" pad="8"/>
<connect gate="B" pin="G" pad="6"/>
<connect gate="B" pin="S" pad="5"/>
<connect gate="C" pin="D" pad="9"/>
<connect gate="C" pin="G" pad="11"/>
<connect gate="C" pin="S" pad="12"/>
<connect gate="D" pin="D" pad="16"/>
<connect gate="D" pin="G" pad="14"/>
<connect gate="D" pin="S" pad="13"/>
<connect gate="P" pin="B" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5205" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="NE5205"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="GND@1" pad="3"/>
<connect gate="A" pin="GND@2" pad="4"/>
<connect gate="A" pin="GND@3" pad="5"/>
<connect gate="A" pin="GND@4" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="VCC@1" pad="1"/>
<connect gate="A" pin="VCC@2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="GND@1" pad="3"/>
<connect gate="A" pin="GND@2" pad="4"/>
<connect gate="A" pin="GND@3" pad="5"/>
<connect gate="A" pin="GND@4" pad="6"/>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="VCC@1" pad="1"/>
<connect gate="A" pin="VCC@2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM340?-*" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM340.pdf</description>
<gates>
<gate name="A" symbol="78XX"/>
</gates>
<devices>
<device name="LZ" package="TO92">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VI" pad="3"/>
<connect gate="A" pin="VO" pad="1"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="H" package="TO220H">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="VI" pad="1"/>
<connect gate="A" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
<device name="MP" package="SOT223">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="VI" pad="1"/>
<connect gate="A" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
</technologies>
</device>
<device name="S" package="TO263-3">
<connects>
<connect gate="A" pin="GND" pad="TAB"/>
<connect gate="A" pin="VI" pad="1"/>
<connect gate="A" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="12"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM320LZ-XX" prefix="IC">
<description>Negative &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="79XX"/>
</gates>
<devices>
<device name="" package="TO92">
<connects>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="VI" pad="2"/>
<connect gate="A" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF01" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="REF02"/>
</gates>
<devices>
<device name="J" package="TO99">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="Z" package="DIL08">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF02" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="REF02"/>
</gates>
<devices>
<device name="J" package="TO99">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="Z" package="DIL08">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD581H" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="78XX"/>
</gates>
<devices>
<device name="" package="TO39">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VI" pad="1"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM311" prefix="IC">
<description>&lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="LM311"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/STR" pad="6"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="GND" pad="1"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="ON/STR" pad="6"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2003" prefix="IC">
<description>&lt;b&gt;AUDIO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+GN"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2008" prefix="IC">
<description>&lt;b&gt;AUDIO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+GN"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2030" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+GN"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2006" prefix="IC">
<description>&lt;b&gt;AUDIO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2040" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="V" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2005" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2005"/>
<gate name="B" symbol="2005A"/>
</gates>
<devices>
<device name="T" package="SIP11">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BTSP" pad="11"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="SVRR" pad="3"/>
<connect gate="A" pin="V+" pad="9"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="BTSP" pad="7"/>
<connect gate="B" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2005T" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2005"/>
<gate name="B" symbol="2005A"/>
</gates>
<devices>
<device name="" package="SIP11">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BTSP" pad="11"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="SVRR" pad="3"/>
<connect gate="A" pin="V+" pad="9"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="BTSP" pad="7"/>
<connect gate="B" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2004" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2005"/>
<gate name="B" symbol="2005A"/>
</gates>
<devices>
<device name="T" package="SIP11">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BTSP" pad="11"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="SVRR" pad="3"/>
<connect gate="A" pin="V+" pad="9"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="BTSP" pad="7"/>
<connect gate="B" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA2009" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2005"/>
<gate name="B" symbol="2005A"/>
</gates>
<devices>
<device name="T" package="SIP11">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="BTSP" pad="11"/>
<connect gate="A" pin="GND" pad="6"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="SVRR" pad="3"/>
<connect gate="A" pin="V+" pad="9"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="BTSP" pad="7"/>
<connect gate="B" pin="OUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM387" prefix="IC">
<description>&lt;b&gt;Low Noise Dual Preamplifier&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+G"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="B" pin="+IN" pad="8"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="B" pin="+IN" pad="8"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE542" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+G"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="B" pin="+IN" pad="8"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="B" pin="+IN" pad="8"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="V+" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L2722" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+G"/>
</gates>
<devices>
<device name="M" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="7"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="5"/>
<connect gate="B" pin="OUT" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="7"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="5"/>
<connect gate="B" pin="OUT" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L272" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+G"/>
</gates>
<devices>
<device name="M" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="7"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="5"/>
<connect gate="B" pin="OUT" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="7"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="5"/>
<connect gate="B" pin="OUT" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DACO8P" prefix="IC">
<description>8-bit &lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="DAC08"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!IO" pad="2"/>
<connect gate="A" pin="+VR" pad="14"/>
<connect gate="A" pin="-VR" pad="15"/>
<connect gate="A" pin="CMP" pad="16"/>
<connect gate="A" pin="D0" pad="5"/>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="9"/>
<connect gate="A" pin="D5" pad="10"/>
<connect gate="A" pin="D6" pad="11"/>
<connect gate="A" pin="D7" pad="12"/>
<connect gate="A" pin="IO" pad="4"/>
<connect gate="A" pin="V+" pad="13"/>
<connect gate="A" pin="V-" pad="3"/>
<connect gate="A" pin="VLC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!IO" pad="2"/>
<connect gate="A" pin="+VR" pad="14"/>
<connect gate="A" pin="-VR" pad="15"/>
<connect gate="A" pin="CMP" pad="16"/>
<connect gate="A" pin="D0" pad="5"/>
<connect gate="A" pin="D1" pad="6"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="9"/>
<connect gate="A" pin="D5" pad="10"/>
<connect gate="A" pin="D6" pad="11"/>
<connect gate="A" pin="D7" pad="12"/>
<connect gate="A" pin="IO" pad="4"/>
<connect gate="A" pin="V+" pad="13"/>
<connect gate="A" pin="V-" pad="3"/>
<connect gate="A" pin="VLC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1403U" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="78XX"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VI" pad="1"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3914N" prefix="IC">
<description>&lt;b&gt;LED DRIVER&lt;/b&gt;&lt;p&gt;
senses analog voltage levels and drives 10 LEDs</description>
<gates>
<gate name="A" symbol="LM3914"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="A" pin="ADJ" pad="8"/>
<connect gate="A" pin="L1" pad="1"/>
<connect gate="A" pin="L10" pad="10"/>
<connect gate="A" pin="L2" pad="18"/>
<connect gate="A" pin="L3" pad="17"/>
<connect gate="A" pin="L4" pad="16"/>
<connect gate="A" pin="L5" pad="15"/>
<connect gate="A" pin="L6" pad="14"/>
<connect gate="A" pin="L7" pad="13"/>
<connect gate="A" pin="L8" pad="12"/>
<connect gate="A" pin="L9" pad="11"/>
<connect gate="A" pin="MDE" pad="9"/>
<connect gate="A" pin="RHI" pad="6"/>
<connect gate="A" pin="RLO" pad="4"/>
<connect gate="A" pin="SIG" pad="5"/>
<connect gate="A" pin="V+" pad="3"/>
<connect gate="A" pin="V-" pad="2"/>
<connect gate="A" pin="VR" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5534" prefix="IC">
<description>&lt;b&gt;LOW-NOISE OPERATIONAL AMPLIFIER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ne5534.pdf</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="5"/>
<connect gate="A" pin="ON" pad="1"/>
<connect gate="A" pin="ON/CMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="5"/>
<connect gate="A" pin="ON" pad="1"/>
<connect gate="A" pin="ON/CMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE5539" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="NE5539"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="14"/>
<connect gate="A" pin="CMP" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="ON/AV" pad="5"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="14"/>
<connect gate="A" pin="CMP" pad="12"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="ON/AV" pad="5"/>
<connect gate="A" pin="OUT" pad="8"/>
<connect gate="A" pin="V+" pad="10"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NE592?8" prefix="IC">
<description>&lt;b&gt;VIDEO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="NE592N8"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="G1A" pad="7"/>
<connect gate="A" pin="G1B" pad="2"/>
<connect gate="A" pin="IN1" pad="8"/>
<connect gate="A" pin="IN2" pad="1"/>
<connect gate="A" pin="OUT1" pad="5"/>
<connect gate="A" pin="OUT2" pad="4"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="G1A" pad="7"/>
<connect gate="A" pin="G1B" pad="2"/>
<connect gate="A" pin="IN1" pad="8"/>
<connect gate="A" pin="IN2" pad="1"/>
<connect gate="A" pin="OUT1" pad="5"/>
<connect gate="A" pin="OUT2" pad="4"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD580H" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;&lt;p&gt;
2.5 V</description>
<gates>
<gate name="A" symbol="78XX"/>
</gates>
<devices>
<device name="" package="TO39">
<connects>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="VI" pad="1"/>
<connect gate="A" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAT-01H" prefix="IC">
<description>Dual &lt;b&gt;TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="NPN-L"/>
<gate name="B" symbol="NPN-R"/>
</gates>
<devices>
<device name="" package="TO78">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="B" pin="B" pad="5"/>
<connect gate="B" pin="C" pad="6"/>
<connect gate="B" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAT-04" prefix="IC">
<description>Quad &lt;b&gt;TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="NPN-L"/>
<gate name="B" symbol="NPN-R"/>
<gate name="C" symbol="NPN-L"/>
<gate name="D" symbol="NPN-R"/>
</gates>
<devices>
<device name="Y" package="DIL14">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="B" pin="B" pad="6"/>
<connect gate="B" pin="C" pad="7"/>
<connect gate="B" pin="E" pad="5"/>
<connect gate="C" pin="B" pad="9"/>
<connect gate="C" pin="C" pad="8"/>
<connect gate="C" pin="E" pad="10"/>
<connect gate="D" pin="B" pad="13"/>
<connect gate="D" pin="C" pad="14"/>
<connect gate="D" pin="E" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="B" pin="B" pad="6"/>
<connect gate="B" pin="C" pad="7"/>
<connect gate="B" pin="E" pad="5"/>
<connect gate="C" pin="B" pad="9"/>
<connect gate="C" pin="C" pad="8"/>
<connect gate="C" pin="E" pad="10"/>
<connect gate="D" pin="B" pad="13"/>
<connect gate="D" pin="C" pad="14"/>
<connect gate="D" pin="E" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAT-02H" prefix="IC">
<description>Dual &lt;b&gt;TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="NPN-L"/>
<gate name="B" symbol="NPN-R"/>
</gates>
<devices>
<device name="" package="TO78">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="B" pin="B" pad="5"/>
<connect gate="B" pin="C" pad="6"/>
<connect gate="B" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF03" prefix="IC">
<description>&lt;b&gt;VOLTAGE REFERENCE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="REF02"/>
</gates>
<devices>
<device name="J" package="TO99">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="Z" package="DIL08">
<connects>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="OPT" pad="3"/>
<connect gate="A" pin="TRM" pad="5"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="A" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1648L" prefix="IC">
<description>&lt;b&gt;VCO&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="MC1648"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="AGC" pad="5"/>
<connect gate="A" pin="BS" pad="10"/>
<connect gate="A" pin="Q" pad="3"/>
<connect gate="A" pin="TNK" pad="12"/>
<connect gate="A" pin="V1+" pad="1"/>
<connect gate="A" pin="V1-" pad="7"/>
<connect gate="A" pin="V2+" pad="14"/>
<connect gate="A" pin="V2-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="AGC" pad="5"/>
<connect gate="A" pin="BS" pad="10"/>
<connect gate="A" pin="Q" pad="3"/>
<connect gate="A" pin="TNK" pad="12"/>
<connect gate="A" pin="V1+" pad="1"/>
<connect gate="A" pin="V1-" pad="7"/>
<connect gate="A" pin="V2+" pad="14"/>
<connect gate="A" pin="V2-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1871N" prefix="IC">
<description>&lt;b&gt;RC TRANSMITTER&lt;/b&gt;&lt;p&gt;
4 channels</description>
<gates>
<gate name="A" symbol="LM1871"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="A" pin="A" pad="5"/>
<connect gate="A" pin="B" pad="6"/>
<connect gate="A" pin="BS" pad="10"/>
<connect gate="A" pin="CH1" pad="3"/>
<connect gate="A" pin="CH2" pad="2"/>
<connect gate="A" pin="CH3" pad="1"/>
<connect gate="A" pin="CH4" pad="18"/>
<connect gate="A" pin="CH5" pad="17"/>
<connect gate="A" pin="CH6" pad="16"/>
<connect gate="A" pin="FRM" pad="7"/>
<connect gate="A" pin="GND" pad="9"/>
<connect gate="A" pin="MF" pad="12"/>
<connect gate="A" pin="MQ" pad="13"/>
<connect gate="A" pin="PLS" pad="8"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="RFQ" pad="11"/>
<connect gate="A" pin="RM" pad="15"/>
<connect gate="A" pin="V+" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1872N" prefix="IC">
<description>&lt;b&gt;RC RECEIVER&lt;/b&gt;&lt;p&gt;
4 channels</description>
<gates>
<gate name="A" symbol="LM1872"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="A" pin="AGC" pad="16"/>
<connect gate="A" pin="GND@1" pad="3"/>
<connect gate="A" pin="GND@2" pad="14"/>
<connect gate="A" pin="IFI" pad="17"/>
<connect gate="A" pin="IFQ" pad="15"/>
<connect gate="A" pin="LO" pad="1"/>
<connect gate="A" pin="MXI" pad="5"/>
<connect gate="A" pin="MXQ" pad="18"/>
<connect gate="A" pin="Q1" pad="11"/>
<connect gate="A" pin="Q2" pad="12"/>
<connect gate="A" pin="QCA" pad="7"/>
<connect gate="A" pin="QCB" pad="9"/>
<connect gate="A" pin="QEA" pad="8"/>
<connect gate="A" pin="QEB" pad="10"/>
<connect gate="A" pin="SYNC" pad="13"/>
<connect gate="A" pin="V+" pad="6"/>
<connect gate="A" pin="VBS" pad="4"/>
<connect gate="A" pin="XTL" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*723" prefix="IC">
<description>Positive &lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="723"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="CL" pad="2"/>
<connect gate="A" pin="CMP" pad="13"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="V+" pad="12"/>
<connect gate="A" pin="V-" pad="7"/>
<connect gate="A" pin="VC" pad="11"/>
<connect gate="A" pin="VZ" pad="9"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="UA"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="5"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="CL" pad="2"/>
<connect gate="A" pin="CMP" pad="13"/>
<connect gate="A" pin="CS" pad="3"/>
<connect gate="A" pin="OUT" pad="10"/>
<connect gate="A" pin="REF" pad="6"/>
<connect gate="A" pin="V+" pad="12"/>
<connect gate="A" pin="V-" pad="7"/>
<connect gate="A" pin="VC" pad="11"/>
<connect gate="A" pin="VZ" pad="9"/>
</connects>
<technologies>
<technology name="LM"/>
<technology name="UA"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0801" prefix="IC">
<description>8-bit &lt;b&gt;A/D CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="ADC0801"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="A" pin="AGND" pad="8"/>
<connect gate="A" pin="CLK" pad="4"/>
<connect gate="A" pin="CLKR" pad="19"/>
<connect gate="A" pin="CS" pad="1"/>
<connect gate="A" pin="DB0" pad="18"/>
<connect gate="A" pin="DB1" pad="17"/>
<connect gate="A" pin="DB2" pad="16"/>
<connect gate="A" pin="DB3" pad="15"/>
<connect gate="A" pin="DB4" pad="14"/>
<connect gate="A" pin="DB5" pad="13"/>
<connect gate="A" pin="DB6" pad="12"/>
<connect gate="A" pin="DB7" pad="11"/>
<connect gate="A" pin="INTR" pad="5"/>
<connect gate="A" pin="RD" pad="2"/>
<connect gate="A" pin="VI+" pad="6"/>
<connect gate="A" pin="VI-" pad="7"/>
<connect gate="A" pin="VREF" pad="9"/>
<connect gate="A" pin="WR" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0808" prefix="IC">
<description>8-bit &lt;b&gt;A/D CONVERTER&lt;/b&gt; with 8-channel multiplexer</description>
<gates>
<gate name="A" symbol="ADC0808"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="N" package="DIL28-6">
<connects>
<connect gate="A" pin="A0" pad="25"/>
<connect gate="A" pin="A1" pad="24"/>
<connect gate="A" pin="A2" pad="23"/>
<connect gate="A" pin="ALE" pad="22"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D0" pad="17"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="18"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="20"/>
<connect gate="A" pin="D7" pad="21"/>
<connect gate="A" pin="EOC" pad="7"/>
<connect gate="A" pin="IN0" pad="26"/>
<connect gate="A" pin="IN1" pad="27"/>
<connect gate="A" pin="IN2" pad="28"/>
<connect gate="A" pin="IN3" pad="1"/>
<connect gate="A" pin="IN4" pad="2"/>
<connect gate="A" pin="IN5" pad="3"/>
<connect gate="A" pin="IN6" pad="4"/>
<connect gate="A" pin="IN7" pad="5"/>
<connect gate="A" pin="OE" pad="9"/>
<connect gate="A" pin="START" pad="6"/>
<connect gate="A" pin="VREF+" pad="12"/>
<connect gate="A" pin="VREF-" pad="16"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO28W">
<connects>
<connect gate="A" pin="A0" pad="25"/>
<connect gate="A" pin="A1" pad="24"/>
<connect gate="A" pin="A2" pad="23"/>
<connect gate="A" pin="ALE" pad="22"/>
<connect gate="A" pin="CLK" pad="10"/>
<connect gate="A" pin="D0" pad="17"/>
<connect gate="A" pin="D1" pad="14"/>
<connect gate="A" pin="D2" pad="15"/>
<connect gate="A" pin="D3" pad="8"/>
<connect gate="A" pin="D4" pad="18"/>
<connect gate="A" pin="D5" pad="19"/>
<connect gate="A" pin="D6" pad="20"/>
<connect gate="A" pin="D7" pad="21"/>
<connect gate="A" pin="EOC" pad="7"/>
<connect gate="A" pin="IN0" pad="26"/>
<connect gate="A" pin="IN1" pad="27"/>
<connect gate="A" pin="IN2" pad="28"/>
<connect gate="A" pin="IN3" pad="1"/>
<connect gate="A" pin="IN4" pad="2"/>
<connect gate="A" pin="IN5" pad="3"/>
<connect gate="A" pin="IN6" pad="4"/>
<connect gate="A" pin="IN7" pad="5"/>
<connect gate="A" pin="OE" pad="9"/>
<connect gate="A" pin="START" pad="6"/>
<connect gate="A" pin="VREF+" pad="12"/>
<connect gate="A" pin="VREF-" pad="16"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="VCC" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC0800" prefix="IC">
<description>8-bit &lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="DAC0800"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="A" pin="!IOUT" pad="2"/>
<connect gate="A" pin="+V" pad="13"/>
<connect gate="A" pin="-V" pad="3"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="B3" pad="7"/>
<connect gate="A" pin="B4" pad="8"/>
<connect gate="A" pin="B5" pad="9"/>
<connect gate="A" pin="B6" pad="10"/>
<connect gate="A" pin="B7" pad="11"/>
<connect gate="A" pin="B8" pad="12"/>
<connect gate="A" pin="COMP" pad="16"/>
<connect gate="A" pin="IOUT" pad="4"/>
<connect gate="A" pin="VLC" pad="1"/>
<connect gate="A" pin="VREF+" pad="14"/>
<connect gate="A" pin="VREF-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="A" pin="!IOUT" pad="2"/>
<connect gate="A" pin="+V" pad="13"/>
<connect gate="A" pin="-V" pad="3"/>
<connect gate="A" pin="B1" pad="5"/>
<connect gate="A" pin="B2" pad="6"/>
<connect gate="A" pin="B3" pad="7"/>
<connect gate="A" pin="B4" pad="8"/>
<connect gate="A" pin="B5" pad="9"/>
<connect gate="A" pin="B6" pad="10"/>
<connect gate="A" pin="B7" pad="11"/>
<connect gate="A" pin="B8" pad="12"/>
<connect gate="A" pin="COMP" pad="16"/>
<connect gate="A" pin="IOUT" pad="4"/>
<connect gate="A" pin="VLC" pad="1"/>
<connect gate="A" pin="VREF+" pad="14"/>
<connect gate="A" pin="VREF-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC0808" prefix="IC">
<description>8-bit &lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/ds/DA/DAC0808.pdf</description>
<gates>
<gate name="P" symbol="2PWRGND"/>
<gate name="P1" symbol="DAC0808"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="13"/>
<connect gate="P" pin="VEE" pad="3"/>
<connect gate="P1" pin="A1" pad="5"/>
<connect gate="P1" pin="A2" pad="6"/>
<connect gate="P1" pin="A3" pad="7"/>
<connect gate="P1" pin="A4" pad="8"/>
<connect gate="P1" pin="A5" pad="9"/>
<connect gate="P1" pin="A6" pad="10"/>
<connect gate="P1" pin="A7" pad="11"/>
<connect gate="P1" pin="A8" pad="12"/>
<connect gate="P1" pin="COMP" pad="16"/>
<connect gate="P1" pin="IOUT" pad="4"/>
<connect gate="P1" pin="VREF+" pad="14"/>
<connect gate="P1" pin="VREF-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="VCC" pad="1"/>
<connect gate="P" pin="VEE" pad="7"/>
<connect gate="P1" pin="A1" pad="9"/>
<connect gate="P1" pin="A2" pad="10"/>
<connect gate="P1" pin="A3" pad="11"/>
<connect gate="P1" pin="A4" pad="12"/>
<connect gate="P1" pin="A5" pad="13"/>
<connect gate="P1" pin="A6" pad="14"/>
<connect gate="P1" pin="A7" pad="15"/>
<connect gate="P1" pin="A8" pad="16"/>
<connect gate="P1" pin="COMP" pad="4"/>
<connect gate="P1" pin="IOUT" pad="8"/>
<connect gate="P1" pin="VREF+" pad="2"/>
<connect gate="P1" pin="VREF-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC0811" prefix="IC">
<description>A/D CONVERTER&lt;/b&gt; with 10-channel multiplexer</description>
<gates>
<gate name="P1" symbol="ADC0811"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
<connect gate="P1" pin="AGND" pad="13"/>
<connect gate="P1" pin="CH0" pad="1"/>
<connect gate="P1" pin="CH1" pad="2"/>
<connect gate="P1" pin="CH10" pad="12"/>
<connect gate="P1" pin="CH2" pad="3"/>
<connect gate="P1" pin="CH3" pad="4"/>
<connect gate="P1" pin="CH4" pad="5"/>
<connect gate="P1" pin="CH5" pad="6"/>
<connect gate="P1" pin="CH6" pad="7"/>
<connect gate="P1" pin="CH7" pad="8"/>
<connect gate="P1" pin="CH8" pad="9"/>
<connect gate="P1" pin="CH9" pad="11"/>
<connect gate="P1" pin="CS" pad="15"/>
<connect gate="P1" pin="D0" pad="16"/>
<connect gate="P1" pin="D1" pad="17"/>
<connect gate="P1" pin="PHI2CLK" pad="19"/>
<connect gate="P1" pin="SCLK" pad="18"/>
<connect gate="P1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA11H" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="T" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA21" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="Z" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA*?" prefix="IC">
<description>&lt;b&gt;Ultra-Low Noise, Precision OP AMP&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa27.pdf&lt;br&gt;
http://focus.ti.com .. opa241.pdf</description>
<gates>
<gate name="G$1" symbol="OP+OFFSET"/>
</gates>
<devices>
<device name="GP" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OFF1" pad="1"/>
<connect gate="G$1" pin="OFF2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="27"/>
<technology name="37"/>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OFF1" pad="1"/>
<connect gate="G$1" pin="OFF2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="27"/>
<technology name="37"/>
</technologies>
</device>
<device name="PA" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OFF1" pad="1"/>
<connect gate="G$1" pin="OFF2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="241"/>
<technology name="251"/>
</technologies>
</device>
<device name="UA" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OFF1" pad="1"/>
<connect gate="G$1" pin="OFF2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="241"/>
<technology name="251"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA10*" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="T" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA111" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="2NUL"/>
</gates>
<devices>
<device name="T" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="ON1" pad="1"/>
<connect gate="A" pin="ON2" pad="5"/>
<connect gate="A" pin="OPT" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA1013" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2107" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="T" package="TO99">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC7*" prefix="IC">
<description>16-bit &lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DAC700"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="G$1" pin="+VCC" pad="23"/>
<connect gate="G$1" pin="-VCC" pad="19"/>
<connect gate="G$1" pin="B1" pad="1"/>
<connect gate="G$1" pin="B10" pad="10"/>
<connect gate="G$1" pin="B11" pad="11"/>
<connect gate="G$1" pin="B12" pad="12"/>
<connect gate="G$1" pin="B13" pad="13"/>
<connect gate="G$1" pin="B14" pad="14"/>
<connect gate="G$1" pin="B15" pad="15"/>
<connect gate="G$1" pin="B16" pad="16"/>
<connect gate="G$1" pin="B2" pad="2"/>
<connect gate="G$1" pin="B3" pad="3"/>
<connect gate="G$1" pin="B4" pad="4"/>
<connect gate="G$1" pin="B5" pad="5"/>
<connect gate="G$1" pin="B6" pad="6"/>
<connect gate="G$1" pin="B7" pad="7"/>
<connect gate="G$1" pin="B8" pad="8"/>
<connect gate="G$1" pin="B9" pad="9"/>
<connect gate="G$1" pin="GAINADJ" pad="22"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="IOUT" pad="21"/>
<connect gate="G$1" pin="REFOUT" pad="24"/>
<connect gate="G$1" pin="RFEEDBCK" pad="17"/>
<connect gate="G$1" pin="VDD" pad="18"/>
</connects>
<technologies>
<technology name="00"/>
<technology name="02"/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="G$1" pin="+VCC" pad="23"/>
<connect gate="G$1" pin="-VCC" pad="19"/>
<connect gate="G$1" pin="B1" pad="1"/>
<connect gate="G$1" pin="B10" pad="10"/>
<connect gate="G$1" pin="B11" pad="11"/>
<connect gate="G$1" pin="B12" pad="12"/>
<connect gate="G$1" pin="B13" pad="13"/>
<connect gate="G$1" pin="B14" pad="14"/>
<connect gate="G$1" pin="B15" pad="15"/>
<connect gate="G$1" pin="B16" pad="16"/>
<connect gate="G$1" pin="B2" pad="2"/>
<connect gate="G$1" pin="B3" pad="3"/>
<connect gate="G$1" pin="B4" pad="4"/>
<connect gate="G$1" pin="B5" pad="5"/>
<connect gate="G$1" pin="B6" pad="6"/>
<connect gate="G$1" pin="B7" pad="7"/>
<connect gate="G$1" pin="B8" pad="8"/>
<connect gate="G$1" pin="B9" pad="9"/>
<connect gate="G$1" pin="GAINADJ" pad="22"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="IOUT" pad="21"/>
<connect gate="G$1" pin="REFOUT" pad="24"/>
<connect gate="G$1" pin="RFEEDBCK" pad="17"/>
<connect gate="G$1" pin="VDD" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DAC70*" prefix="IC">
<description>16-bit &lt;b&gt;DIGITAL/ANALOG CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DAC701"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="G$1" pin="+VCC" pad="23"/>
<connect gate="G$1" pin="-VCC" pad="19"/>
<connect gate="G$1" pin="B1" pad="1"/>
<connect gate="G$1" pin="B10" pad="10"/>
<connect gate="G$1" pin="B11" pad="11"/>
<connect gate="G$1" pin="B12" pad="12"/>
<connect gate="G$1" pin="B13" pad="13"/>
<connect gate="G$1" pin="B14" pad="14"/>
<connect gate="G$1" pin="B15" pad="15"/>
<connect gate="G$1" pin="B16" pad="16"/>
<connect gate="G$1" pin="B2" pad="2"/>
<connect gate="G$1" pin="B3" pad="3"/>
<connect gate="G$1" pin="B4" pad="4"/>
<connect gate="G$1" pin="B5" pad="5"/>
<connect gate="G$1" pin="B6" pad="6"/>
<connect gate="G$1" pin="B7" pad="7"/>
<connect gate="G$1" pin="B8" pad="8"/>
<connect gate="G$1" pin="B9" pad="9"/>
<connect gate="G$1" pin="GAINADJ" pad="22"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="REFOUT" pad="24"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VOUT" pad="17"/>
<connect gate="G$1" pin="ZEROADJ" pad="21"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="3"/>
</technologies>
</device>
<device name="D" package="SO24W">
<connects>
<connect gate="G$1" pin="+VCC" pad="23"/>
<connect gate="G$1" pin="-VCC" pad="19"/>
<connect gate="G$1" pin="B1" pad="1"/>
<connect gate="G$1" pin="B10" pad="10"/>
<connect gate="G$1" pin="B11" pad="11"/>
<connect gate="G$1" pin="B12" pad="12"/>
<connect gate="G$1" pin="B13" pad="13"/>
<connect gate="G$1" pin="B14" pad="14"/>
<connect gate="G$1" pin="B15" pad="15"/>
<connect gate="G$1" pin="B16" pad="16"/>
<connect gate="G$1" pin="B2" pad="2"/>
<connect gate="G$1" pin="B3" pad="3"/>
<connect gate="G$1" pin="B4" pad="4"/>
<connect gate="G$1" pin="B5" pad="5"/>
<connect gate="G$1" pin="B6" pad="6"/>
<connect gate="G$1" pin="B7" pad="7"/>
<connect gate="G$1" pin="B8" pad="8"/>
<connect gate="G$1" pin="B9" pad="9"/>
<connect gate="G$1" pin="GAINADJ" pad="22"/>
<connect gate="G$1" pin="GND" pad="20"/>
<connect gate="G$1" pin="REFOUT" pad="24"/>
<connect gate="G$1" pin="VDD" pad="18"/>
<connect gate="G$1" pin="VOUT" pad="17"/>
<connect gate="G$1" pin="ZEROADJ" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDM862" prefix="IC">
<description>&lt;b&gt;DATA ACQUSITION SYSTEM&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SDM862"/>
</gates>
<devices>
<device name="" package="PGA68">
<connects>
<connect gate="G$1" pin="!CS" pad="31"/>
<connect gate="G$1" pin="+15(1)" pad="3"/>
<connect gate="G$1" pin="+15(2)" pad="27"/>
<connect gate="G$1" pin="+5V(2)" pad="5"/>
<connect gate="G$1" pin="-15(1)" pad="4"/>
<connect gate="G$1" pin="-15(2)" pad="20"/>
<connect gate="G$1" pin="ACOM(2)" pad="25"/>
<connect gate="G$1" pin="ADCIN_10" pad="22"/>
<connect gate="G$1" pin="ADCIN_20" pad="21"/>
<connect gate="G$1" pin="AMP_IN-" pad="66"/>
<connect gate="G$1" pin="AMP_OUT" pad="1"/>
<connect gate="G$1" pin="AMP_REF" pad="2"/>
<connect gate="G$1" pin="AMP_SENS" pad="68"/>
<connect gate="G$1" pin="BIP_OFF" pad="23"/>
<connect gate="G$1" pin="BYTE_SEL" pad="32"/>
<connect gate="G$1" pin="CE" pad="28"/>
<connect gate="G$1" pin="CH0" pad="47"/>
<connect gate="G$1" pin="CH1" pad="46"/>
<connect gate="G$1" pin="CH10" pad="56"/>
<connect gate="G$1" pin="CH11" pad="57"/>
<connect gate="G$1" pin="CH12" pad="58"/>
<connect gate="G$1" pin="CH13" pad="59"/>
<connect gate="G$1" pin="CH14" pad="60"/>
<connect gate="G$1" pin="CH15" pad="61"/>
<connect gate="G$1" pin="CH2" pad="45"/>
<connect gate="G$1" pin="CH3" pad="44"/>
<connect gate="G$1" pin="CH4" pad="43"/>
<connect gate="G$1" pin="CH5" pad="42"/>
<connect gate="G$1" pin="CH6" pad="41"/>
<connect gate="G$1" pin="CH7" pad="40"/>
<connect gate="G$1" pin="CH8" pad="54"/>
<connect gate="G$1" pin="CH9" pad="55"/>
<connect gate="G$1" pin="D0" pad="18"/>
<connect gate="G$1" pin="D1" pad="17"/>
<connect gate="G$1" pin="D10" pad="8"/>
<connect gate="G$1" pin="D11" pad="7"/>
<connect gate="G$1" pin="D2" pad="16"/>
<connect gate="G$1" pin="D3" pad="15"/>
<connect gate="G$1" pin="D4" pad="14"/>
<connect gate="G$1" pin="D5" pad="13"/>
<connect gate="G$1" pin="D6" pad="12"/>
<connect gate="G$1" pin="D7" pad="11"/>
<connect gate="G$1" pin="D8" pad="10"/>
<connect gate="G$1" pin="D9" pad="9"/>
<connect gate="G$1" pin="DATA_MOD" pad="30"/>
<connect gate="G$1" pin="DCOM(1)" pad="53"/>
<connect gate="G$1" pin="DCOM(2)" pad="19"/>
<connect gate="G$1" pin="G10" pad="63"/>
<connect gate="G$1" pin="G100" pad="64"/>
<connect gate="G$1" pin="HOLD_CAP" pad="36"/>
<connect gate="G$1" pin="MO+/AMP+" pad="65"/>
<connect gate="G$1" pin="MUX_ADD0" pad="49"/>
<connect gate="G$1" pin="MUX_ADD1" pad="50"/>
<connect gate="G$1" pin="MUX_ADD2" pad="51"/>
<connect gate="G$1" pin="MUX_ADD3" pad="52"/>
<connect gate="G$1" pin="MUX_ENA" pad="48"/>
<connect gate="G$1" pin="NC1" pad="38"/>
<connect gate="G$1" pin="NC2" pad="67"/>
<connect gate="G$1" pin="R/!C" pad="29"/>
<connect gate="G$1" pin="REF_IN" pad="24"/>
<connect gate="G$1" pin="REF_OUT" pad="26"/>
<connect gate="G$1" pin="RG" pad="62"/>
<connect gate="G$1" pin="S/H_COM2" pad="34"/>
<connect gate="G$1" pin="S/H_CONT" pad="33"/>
<connect gate="G$1" pin="S/H_IN" pad="39"/>
<connect gate="G$1" pin="S/H_O@1" pad="37"/>
<connect gate="G$1" pin="S/H_O@2" pad="35"/>
<connect gate="G$1" pin="STATUS" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD524" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD524"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="10" pad="13"/>
<connect gate="G$1" pin="100" pad="12"/>
<connect gate="G$1" pin="1000" pad="11"/>
<connect gate="G$1" pin="I-N1" pad="4"/>
<connect gate="G$1" pin="I-N2" pad="5"/>
<connect gate="G$1" pin="O-N1" pad="14"/>
<connect gate="G$1" pin="O-N2" pad="15"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="RG1" pad="16"/>
<connect gate="G$1" pin="RG2" pad="3"/>
<connect gate="G$1" pin="SENS" pad="10"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="10" pad="13"/>
<connect gate="G$1" pin="100" pad="12"/>
<connect gate="G$1" pin="1000" pad="11"/>
<connect gate="G$1" pin="I-N1" pad="4"/>
<connect gate="G$1" pin="I-N2" pad="5"/>
<connect gate="G$1" pin="O-N1" pad="14"/>
<connect gate="G$1" pin="O-N2" pad="15"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="REF" pad="6"/>
<connect gate="G$1" pin="RG1" pad="16"/>
<connect gate="G$1" pin="RG2" pad="3"/>
<connect gate="G$1" pin="SENS" pad="10"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MAT-03H" prefix="IC">
<description>Dual &lt;b&gt;TRANSISTOR&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PNP-L"/>
<gate name="B" symbol="PNP-R"/>
</gates>
<devices>
<device name="" package="TO78">
<connects>
<connect gate="A" pin="B" pad="2"/>
<connect gate="A" pin="C" pad="1"/>
<connect gate="A" pin="E" pad="3"/>
<connect gate="B" pin="B" pad="5"/>
<connect gate="B" pin="C" pad="6"/>
<connect gate="B" pin="E" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SSM2402" prefix="IC">
<description>&lt;b&gt;ANALOG SWITCH&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="SSM2402"/>
<gate name="B" symbol="SSM2402"/>
<gate name="P" symbol="PWR+-GR"/>
</gates>
<devices>
<device name="S" package="SO16L">
<connects>
<connect gate="A" pin="CTL" pad="2"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="B" pin="CTL" pad="15"/>
<connect gate="B" pin="IN" pad="13"/>
<connect gate="B" pin="OUT" pad="11"/>
<connect gate="P" pin="GND" pad="1"/>
<connect gate="P" pin="V+" pad="16"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="CTL" pad="2"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="B" pin="CTL" pad="13"/>
<connect gate="B" pin="IN" pad="11"/>
<connect gate="B" pin="OUT" pad="9"/>
<connect gate="P" pin="GND" pad="1"/>
<connect gate="P" pin="V+" pad="14"/>
<connect gate="P" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM6325H" prefix="IC">
<description>&lt;b&gt;BUFFER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LM6325"/>
</gates>
<devices>
<device name="" package="TO99">
<connects>
<connect gate="G$1" pin="FLG" pad="5"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="S/D" pad="7"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA134" prefix="IC">
<description>&lt;b&gt;AUDIO AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="2NUL"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="ON1" pad="1"/>
<connect gate="G$1" pin="ON2" pad="8"/>
<connect gate="G$1" pin="OPT" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="ON1" pad="1"/>
<connect gate="G$1" pin="ON2" pad="8"/>
<connect gate="G$1" pin="OPT" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD797" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="2NUL"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="ON1" pad="1"/>
<connect gate="G$1" pin="ON2" pad="5"/>
<connect gate="G$1" pin="OPT" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="ON1" pad="1"/>
<connect gate="G$1" pin="ON2" pad="5"/>
<connect gate="G$1" pin="OPT" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L165ST" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP+GN"/>
</gates>
<devices>
<device name="" package="CB360">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM12" prefix="IC">
<description>Power &lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="" package="K04A">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="5 5/" route="any"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RC4136FK" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="E" symbol="PWR+-"/>
<gate name="1" symbol="NC_PIN"/>
<gate name="5" symbol="NC_PIN"/>
<gate name="7" symbol="NC_PIN"/>
<gate name="11" symbol="NC_PIN"/>
<gate name="15" symbol="NC_PIN"/>
<gate name="17" symbol="NC_PIN"/>
</gates>
<devices>
<device name="" package="PLCC20S">
<connects>
<connect gate="1" pin="NC" pad="1"/>
<connect gate="11" pin="NC" pad="11"/>
<connect gate="15" pin="NC" pad="15"/>
<connect gate="17" pin="NC" pad="17"/>
<connect gate="5" pin="NC" pad="5"/>
<connect gate="7" pin="NC" pad="7"/>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="B" pin="+IN" pad="8"/>
<connect gate="B" pin="-IN" pad="9"/>
<connect gate="B" pin="OUT" pad="6"/>
<connect gate="C" pin="+IN" pad="13"/>
<connect gate="C" pin="-IN" pad="12"/>
<connect gate="C" pin="OUT" pad="14"/>
<connect gate="D" pin="+IN" pad="19"/>
<connect gate="D" pin="-IN" pad="20"/>
<connect gate="D" pin="OUT" pad="18"/>
<connect gate="E" pin="V+" pad="16"/>
<connect gate="E" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD22050" prefix="IC">
<description>Sensor interface &lt;b&gt;AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="AD22050"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="8"/>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OFS" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="8"/>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OFS" pad="7"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP262G" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP262" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="HRU" package="TSSOP8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP462" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="GS" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="GP" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="HRU" package="TSSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596S" prefix="IC" uservalue="yes">
<description>&lt;b&gt;STEP-DOWN VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LM2596"/>
</gates>
<devices>
<device name="" package="TO263-5">
<connects>
<connect gate="G$1" pin="EN" pad="5"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2596T" prefix="IC" uservalue="yes">
<description>&lt;b&gt;STEP-DOWN VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="NC1" symbol="LM2596-5"/>
</gates>
<devices>
<device name="V" package="TO220-51">
<connects>
<connect gate="NC1" pin="EN" pad="5"/>
<connect gate="NC1" pin="FB" pad="4"/>
<connect gate="NC1" pin="GND" pad="3"/>
<connect gate="NC1" pin="IN" pad="1"/>
<connect gate="NC1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="H" package="TO220-52">
<connects>
<connect gate="NC1" pin="EN" pad="5"/>
<connect gate="NC1" pin="FB" pad="4"/>
<connect gate="NC1" pin="GND" pad="3"/>
<connect gate="NC1" pin="IN" pad="1"/>
<connect gate="NC1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF398A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;SAMPLE&amp;HOLD AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LF198"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="!SH" pad="8"/>
<connect gate="G$1" pin="CHOLD" pad="6"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="LOGREF" pad="7"/>
<connect gate="G$1" pin="OFFSET" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="!SH" pad="8"/>
<connect gate="G$1" pin="CHOLD" pad="6"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="LOGREF" pad="7"/>
<connect gate="G$1" pin="OFFSET" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF198H" prefix="IC" uservalue="yes">
<description>&lt;b&gt;SAMPLE&amp;HOLD AMPLIFIER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LF198"/>
</gates>
<devices>
<device name="" package="H08C">
<connects>
<connect gate="G$1" pin="!SH" pad="8"/>
<connect gate="G$1" pin="CHOLD" pad="6"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="LOGREF" pad="7"/>
<connect gate="G$1" pin="OFFSET" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78L*SMD" prefix="IC">
<description>&lt;b&gt;Positive VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="LM78LXX"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="3"/>
<connect gate="G$1" pin="GND@3" pad="6"/>
<connect gate="G$1" pin="GND@4" pad="7"/>
<connect gate="G$1" pin="VIN" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="NC4" pin="NC" pad="4"/>
<connect gate="NC5" pin="NC" pad="5"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="06"/>
<technology name="08"/>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="24"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08031" prefix="IC">
<description>A/D CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADC08031"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="CLK" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D0" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VIN+" pad="2"/>
<connect gate="G$1" pin="VIN-" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="CLK" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D0" pad="6"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VIN+" pad="2"/>
<connect gate="G$1" pin="VIN-" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08038" prefix="IC" uservalue="yes">
<description>A/D CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADC08038"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="G$1" pin="AGND" pad="11"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="COM" pad="9"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="D0" pad="14"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="DI" pad="17"/>
<connect gate="G$1" pin="SARS" pad="15"/>
<connect gate="G$1" pin="SE" pad="13"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VREF_I" pad="12"/>
<connect gate="G$1" pin="VREF_O" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO20W">
<connects>
<connect gate="G$1" pin="AGND" pad="11"/>
<connect gate="G$1" pin="CH0" pad="1"/>
<connect gate="G$1" pin="CH1" pad="2"/>
<connect gate="G$1" pin="CH2" pad="3"/>
<connect gate="G$1" pin="CH3" pad="4"/>
<connect gate="G$1" pin="CH4" pad="5"/>
<connect gate="G$1" pin="CH5" pad="6"/>
<connect gate="G$1" pin="CH6" pad="7"/>
<connect gate="G$1" pin="CH7" pad="8"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="COM" pad="9"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="D0" pad="14"/>
<connect gate="G$1" pin="DGND" pad="10"/>
<connect gate="G$1" pin="DI" pad="17"/>
<connect gate="G$1" pin="SARS" pad="15"/>
<connect gate="G$1" pin="SE" pad="13"/>
<connect gate="G$1" pin="VCC" pad="20"/>
<connect gate="G$1" pin="VREF_I" pad="12"/>
<connect gate="G$1" pin="VREF_O" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08034" prefix="IC" uservalue="yes">
<description>A/D CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADC08034"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="G$1" pin="AGND" pad="8"/>
<connect gate="G$1" pin="CH0" pad="3"/>
<connect gate="G$1" pin="CH1" pad="4"/>
<connect gate="G$1" pin="CH2" pad="5"/>
<connect gate="G$1" pin="CH3" pad="6"/>
<connect gate="G$1" pin="CLK" pad="12"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="D0" pad="10"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DI" pad="13"/>
<connect gate="G$1" pin="SARS" pad="11"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VREF_I" pad="9"/>
<connect gate="G$1" pin="VREF_O" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="G$1" pin="AGND" pad="8"/>
<connect gate="G$1" pin="CH0" pad="3"/>
<connect gate="G$1" pin="CH1" pad="4"/>
<connect gate="G$1" pin="CH2" pad="5"/>
<connect gate="G$1" pin="CH3" pad="6"/>
<connect gate="G$1" pin="CLK" pad="12"/>
<connect gate="G$1" pin="CS" pad="2"/>
<connect gate="G$1" pin="D0" pad="10"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DI" pad="13"/>
<connect gate="G$1" pin="SARS" pad="11"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VREF_I" pad="9"/>
<connect gate="G$1" pin="VREF_O" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC08032" prefix="IC">
<description>A/D CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADC08032"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="CH0" pad="2"/>
<connect gate="G$1" pin="CH1" pad="3"/>
<connect gate="G$1" pin="CLK" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D0" pad="6"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="CH0" pad="2"/>
<connect gate="G$1" pin="CH1" pad="3"/>
<connect gate="G$1" pin="CLK" pad="7"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D0" pad="6"/>
<connect gate="G$1" pin="DI" pad="5"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO14W">
<connects>
<connect gate="G$1" pin="CH0" pad="3"/>
<connect gate="G$1" pin="CH1" pad="5"/>
<connect gate="G$1" pin="CLK" pad="12"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D0" pad="10"/>
<connect gate="G$1" pin="DI" pad="8"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADC8031S" prefix="IC" uservalue="yes">
<description>A/D CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="ADC08031"/>
<gate name="2" symbol="NC"/>
<gate name="4" symbol="NC"/>
<gate name="6" symbol="NC"/>
<gate name="9" symbol="NC"/>
<gate name="11" symbol="NC"/>
<gate name="13" symbol="NC"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="11" pin="NC" pad="11"/>
<connect gate="13" pin="NC" pad="13"/>
<connect gate="2" pin="NC" pad="2"/>
<connect gate="4" pin="NC" pad="4"/>
<connect gate="6" pin="NC" pad="6"/>
<connect gate="9" pin="NC" pad="9"/>
<connect gate="G$1" pin="CLK" pad="12"/>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="D0" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="VIN+" pad="3"/>
<connect gate="G$1" pin="VIN-" pad="5"/>
<connect gate="G$1" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA8501" prefix="IC">
<description>&lt;b&gt;PAL/NTSC encoder&lt;/b&gt;&lt;p&gt;
 Philips Semiconductors</description>
<gates>
<gate name="G$1" symbol="TDA8501"/>
<gate name="P" symbol="VCCVSS"/>
</gates>
<devices>
<device name="T" package="SO24W">
<connects>
<connect gate="G$1" pin="-(B-Y)" pad="3"/>
<connect gate="G$1" pin="-(R-Y)" pad="1"/>
<connect gate="G$1" pin="BLUE" pad="11"/>
<connect gate="G$1" pin="BURSTADJ" pad="21"/>
<connect gate="G$1" pin="CHROMA" pad="14"/>
<connect gate="G$1" pin="CS" pad="24"/>
<connect gate="G$1" pin="CVBS" pad="16"/>
<connect gate="G$1" pin="FLT" pad="15"/>
<connect gate="G$1" pin="GREEN" pad="9"/>
<connect gate="G$1" pin="H/2" pad="4"/>
<connect gate="G$1" pin="MCONTROL" pad="2"/>
<connect gate="G$1" pin="NOTCH" pad="18"/>
<connect gate="G$1" pin="OSC" pad="23"/>
<connect gate="G$1" pin="PAL/NTSC-Y/Y+SYNC" pad="17"/>
<connect gate="G$1" pin="RED" pad="7"/>
<connect gate="G$1" pin="UOFFSET" pad="6"/>
<connect gate="G$1" pin="VOFFSET" pad="12"/>
<connect gate="G$1" pin="VREF" pad="13"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Y+SYNCIN" pad="20"/>
<connect gate="G$1" pin="Y+SYNCOUT1V" pad="22"/>
<connect gate="G$1" pin="Y+SYNCOUT2V" pad="19"/>
<connect gate="P" pin="VCC" pad="8"/>
<connect gate="P" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="-(B-Y)" pad="3"/>
<connect gate="G$1" pin="-(R-Y)" pad="1"/>
<connect gate="G$1" pin="BLUE" pad="11"/>
<connect gate="G$1" pin="BURSTADJ" pad="21"/>
<connect gate="G$1" pin="CHROMA" pad="14"/>
<connect gate="G$1" pin="CS" pad="24"/>
<connect gate="G$1" pin="CVBS" pad="16"/>
<connect gate="G$1" pin="FLT" pad="15"/>
<connect gate="G$1" pin="GREEN" pad="9"/>
<connect gate="G$1" pin="H/2" pad="4"/>
<connect gate="G$1" pin="MCONTROL" pad="2"/>
<connect gate="G$1" pin="NOTCH" pad="18"/>
<connect gate="G$1" pin="OSC" pad="23"/>
<connect gate="G$1" pin="PAL/NTSC-Y/Y+SYNC" pad="17"/>
<connect gate="G$1" pin="RED" pad="7"/>
<connect gate="G$1" pin="UOFFSET" pad="6"/>
<connect gate="G$1" pin="VOFFSET" pad="12"/>
<connect gate="G$1" pin="VREF" pad="13"/>
<connect gate="G$1" pin="Y" pad="5"/>
<connect gate="G$1" pin="Y+SYNCIN" pad="20"/>
<connect gate="G$1" pin="Y+SYNCOUT1V" pad="22"/>
<connect gate="G$1" pin="Y+SYNCOUT2V" pad="19"/>
<connect gate="P" pin="VCC" pad="8"/>
<connect gate="P" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAA1101" prefix="IC">
<description>&lt;b&gt;Universal sync generator (USG)&lt;/b&gt;&lt;p&gt;
Philips Semiconductors</description>
<gates>
<gate name="G$1" symbol="SAA1101"/>
<gate name="P" symbol="VDDVSS"/>
</gates>
<devices>
<device name="T" package="SO28W">
<connects>
<connect gate="G$1" pin="BK" pad="16"/>
<connect gate="G$1" pin="CB" pad="17"/>
<connect gate="G$1" pin="CLO" pad="24"/>
<connect gate="G$1" pin="CLP" pad="19"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="CS0" pad="4"/>
<connect gate="G$1" pin="CS1" pad="3"/>
<connect gate="G$1" pin="ECS" pad="11"/>
<connect gate="G$1" pin="FSI" pad="1"/>
<connect gate="G$1" pin="FSO" pad="2"/>
<connect gate="G$1" pin="HD" pad="22"/>
<connect gate="G$1" pin="ID" pad="15"/>
<connect gate="G$1" pin="LM0" pad="10"/>
<connect gate="G$1" pin="LM1" pad="9"/>
<connect gate="G$1" pin="NORM" pad="23"/>
<connect gate="G$1" pin="OSCI" pad="5"/>
<connect gate="G$1" pin="OSCO" pad="6"/>
<connect gate="G$1" pin="PH" pad="8"/>
<connect gate="G$1" pin="RR" pad="12"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="VD" pad="21"/>
<connect gate="G$1" pin="VLE" pad="7"/>
<connect gate="G$1" pin="WMP" pad="20"/>
<connect gate="G$1" pin="X" pad="25"/>
<connect gate="G$1" pin="Y" pad="26"/>
<connect gate="G$1" pin="Z" pad="27"/>
<connect gate="P" pin="VDD" pad="28"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="BK" pad="16"/>
<connect gate="G$1" pin="CB" pad="17"/>
<connect gate="G$1" pin="CLO" pad="24"/>
<connect gate="G$1" pin="CLP" pad="19"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="CS0" pad="4"/>
<connect gate="G$1" pin="CS1" pad="3"/>
<connect gate="G$1" pin="ECS" pad="11"/>
<connect gate="G$1" pin="FSI" pad="1"/>
<connect gate="G$1" pin="FSO" pad="2"/>
<connect gate="G$1" pin="HD" pad="22"/>
<connect gate="G$1" pin="ID" pad="15"/>
<connect gate="G$1" pin="LM0" pad="10"/>
<connect gate="G$1" pin="LM1" pad="9"/>
<connect gate="G$1" pin="NORM" pad="23"/>
<connect gate="G$1" pin="OSCI" pad="5"/>
<connect gate="G$1" pin="OSCO" pad="6"/>
<connect gate="G$1" pin="PH" pad="8"/>
<connect gate="G$1" pin="RR" pad="12"/>
<connect gate="G$1" pin="SI" pad="13"/>
<connect gate="G$1" pin="VD" pad="21"/>
<connect gate="G$1" pin="VLE" pad="7"/>
<connect gate="G$1" pin="WMP" pad="20"/>
<connect gate="G$1" pin="X" pad="25"/>
<connect gate="G$1" pin="Y" pad="26"/>
<connect gate="G$1" pin="Z" pad="27"/>
<connect gate="P" pin="VDD" pad="28"/>
<connect gate="P" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34119" prefix="IC">
<description>&lt;b&gt;Low Power Audio Amplifier&lt;/b&gt; Motorola</description>
<gates>
<gate name="G$1" symbol="MC34119"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="CD" pad="1"/>
<connect gate="G$1" pin="FC1" pad="3"/>
<connect gate="G$1" pin="FC2" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VO1" pad="5"/>
<connect gate="G$1" pin="VO2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CD" pad="1"/>
<connect gate="G$1" pin="FC1" pad="3"/>
<connect gate="G$1" pin="FC2" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VO1" pad="5"/>
<connect gate="G$1" pin="VO2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DTB" package="TSSOP8">
<connects>
<connect gate="G$1" pin="CD" pad="1"/>
<connect gate="G$1" pin="FC1" pad="3"/>
<connect gate="G$1" pin="FC2" pad="2"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VO1" pad="5"/>
<connect gate="G$1" pin="VO2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4658" prefix="IC">
<description>&lt;b&gt;Quad Wideband, Low Power Current Feedback OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM331*" prefix="IC">
<description>&lt;b&gt;Simple Stand-Alone Voltage-to-Frequency Converter&lt;/b&gt; LM231&lt;p&gt;
with ±0.03% Typical Linearity (f = 10 Hz to 11 kHz)</description>
<gates>
<gate name="G$1" symbol="LM331"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="7"/>
<connect gate="G$1" pin="F-OUT" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="I-OUT" pad="1"/>
<connect gate="G$1" pin="I-REF" pad="2"/>
<connect gate="G$1" pin="RC" pad="5"/>
<connect gate="G$1" pin="THR" pad="6"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1562" prefix="IC">
<description>&lt;b&gt;70 W High Efficiency Power Amplifier&lt;/b&gt;&lt;p&gt;
with diagnostic facility</description>
<gates>
<gate name="G$1" symbol="TDA1562"/>
</gates>
<devices>
<device name="Q" package="MULTIWAT-SIL17">
<connects>
<connect gate="G$1" pin="C1+" pad="5"/>
<connect gate="G$1" pin="C1-" pad="3"/>
<connect gate="G$1" pin="C2+" pad="13"/>
<connect gate="G$1" pin="C2-" pad="15"/>
<connect gate="G$1" pin="DIAGNOSTIC" pad="8"/>
<connect gate="G$1" pin="IN+" pad="1"/>
<connect gate="G$1" pin="IN-" pad="2"/>
<connect gate="G$1" pin="M-SEL" pad="4"/>
<connect gate="G$1" pin="OUT+" pad="7"/>
<connect gate="G$1" pin="OUT-" pad="11"/>
<connect gate="G$1" pin="PGND1" pad="6"/>
<connect gate="G$1" pin="PGND2" pad="12"/>
<connect gate="G$1" pin="SIG-GND" pad="17"/>
<connect gate="G$1" pin="STATUS_IO" pad="16"/>
<connect gate="G$1" pin="VP1" pad="9"/>
<connect gate="G$1" pin="VP2" pad="10"/>
<connect gate="G$1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1560Q" prefix="IC">
<description>&lt;b&gt;40 W car radio high power amplifier&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TDA1560Q"/>
</gates>
<devices>
<device name="" package="MULTIWAT-SIL17">
<connects>
<connect gate="G$1" pin="C1+" pad="10"/>
<connect gate="G$1" pin="C1-" pad="13"/>
<connect gate="G$1" pin="C2+" pad="8"/>
<connect gate="G$1" pin="C2-" pad="5"/>
<connect gate="G$1" pin="CDEC" pad="15"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="INPN" pad="2"/>
<connect gate="G$1" pin="INPP" pad="1"/>
<connect gate="G$1" pin="MODE" pad="16"/>
<connect gate="G$1" pin="OUT1N" pad="7"/>
<connect gate="G$1" pin="OUT2P" pad="11"/>
<connect gate="G$1" pin="S1" pad="17"/>
<connect gate="G$1" pin="SIG-GND" pad="3"/>
<connect gate="G$1" pin="VDIAG" pad="14"/>
<connect gate="G$1" pin="VP" pad="9"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL494*" prefix="IC">
<description>&lt;b&gt;SWITCHMODE Pulse Width Modulation Control Circuit&lt;/b&gt;&lt;p&gt;
NCV494B&lt;br&gt;
http://onsemi.com tl494-d.pdf</description>
<gates>
<gate name="G$1" symbol="TL494"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="+I1" pad="1"/>
<connect gate="G$1" pin="+I2" pad="16"/>
<connect gate="G$1" pin="-I1" pad="2"/>
<connect gate="G$1" pin="-I2" pad="15"/>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="C2" pad="11"/>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="CT" pad="5"/>
<connect gate="G$1" pin="DTC" pad="4"/>
<connect gate="G$1" pin="E1" pad="9"/>
<connect gate="G$1" pin="E2" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUTC" pad="13"/>
<connect gate="G$1" pin="RT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="I"/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="G$1" pin="+I1" pad="1"/>
<connect gate="G$1" pin="+I2" pad="16"/>
<connect gate="G$1" pin="-I1" pad="2"/>
<connect gate="G$1" pin="-I2" pad="15"/>
<connect gate="G$1" pin="C1" pad="8"/>
<connect gate="G$1" pin="C2" pad="11"/>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="CT" pad="5"/>
<connect gate="G$1" pin="DTC" pad="4"/>
<connect gate="G$1" pin="E1" pad="9"/>
<connect gate="G$1" pin="E2" pad="10"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUTC" pad="13"/>
<connect gate="G$1" pin="RT" pad="6"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VREF" pad="14"/>
</connects>
<technologies>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA1516BQ" prefix="IC">
<description>&lt;b&gt;radio power amplifier&lt;/b&gt;&lt;p&gt;
24 W BTL or 2 x 12 watt stereo car&lt;br&gt;
Source: TDA1516BQ_1.pdf</description>
<gates>
<gate name="G$1" symbol="TDA1516"/>
</gates>
<devices>
<device name="" package="MULTIWAT-SIL13">
<connects>
<connect gate="G$1" pin="GNDP" pad="7"/>
<connect gate="G$1" pin="GNDS" pad="3"/>
<connect gate="G$1" pin="IN1+" pad="1"/>
<connect gate="G$1" pin="IN1-" pad="2"/>
<connect gate="G$1" pin="IN2+" pad="13"/>
<connect gate="G$1" pin="INT_VP1/2" pad="12"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="9"/>
<connect gate="G$1" pin="STDBY" pad="11"/>
<connect gate="G$1" pin="VP" pad="10"/>
<connect gate="G$1" pin="VP1" pad="6"/>
<connect gate="G$1" pin="VP2" pad="8"/>
<connect gate="G$1" pin="VREF" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM*34" prefix="IC">
<description>&lt;b&gt;3-Terminal Adjustable Current Sources&lt;/b&gt;&lt;br&gt;
Source: www.national.com/pf/LM/LM334.html | LM134.pdf</description>
<gates>
<gate name="G$1" symbol="ACS"/>
</gates>
<devices>
<device name="Z" package="TO92">
<connects>
<connect gate="G$1" pin="R" pad="2"/>
<connect gate="G$1" pin="V+" pad="1"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="2"/>
<technology name="3"/>
</technologies>
</device>
<device name="SM" package="SO08">
<connects>
<connect gate="G$1" pin="R" pad="2"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="1"/>
</connects>
<technologies>
<technology name="3"/>
</technologies>
</device>
<device name="H" package="TO46">
<connects>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="3"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
<technology name="3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM334*" prefix="IC">
<description>&lt;b&gt;3-Terminal Adjustable Current Sources&lt;/b&gt;&lt;br&gt;
Source: www.national.com/pf/LM/LM334.html | LM134.pdf</description>
<gates>
<gate name="G$1" symbol="LM334-2"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="R" pad="1"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="2"/>
<connect gate="G$1" pin="V-@1" pad="3"/>
<connect gate="G$1" pin="V-@2" pad="6"/>
<connect gate="G$1" pin="V-@3" pad="7"/>
</connects>
<technologies>
<technology name="M"/>
<technology name="MX"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLA706*M" prefix="IC">
<description>&lt;b&gt;UNIPOLAR STEPPER-MOTOR TRANSLATOR/DRIVERS&lt;/b&gt;&lt;p&gt;
Source: www.allegromicro.com .. 97060.pdf</description>
<gates>
<gate name="G$1" symbol="SLA706"/>
</gates>
<devices>
<device name="" package="ZIP21-SLA">
<connects>
<connect gate="G$1" pin="!OUTA" pad="3"/>
<connect gate="G$1" pin="!OUTA@1" pad="4"/>
<connect gate="G$1" pin="!OUTB" pad="19"/>
<connect gate="G$1" pin="!OUTB@1" pad="18"/>
<connect gate="G$1" pin="CLOCK" pad="10"/>
<connect gate="G$1" pin="CW/CCW" pad="9"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="M0" pad="14"/>
<connect gate="G$1" pin="M1" pad="13"/>
<connect gate="G$1" pin="M2" pad="12"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTA@1" pad="1"/>
<connect gate="G$1" pin="OUTB" pad="20"/>
<connect gate="G$1" pin="OUTB@1" pad="21"/>
<connect gate="G$1" pin="REF" pad="7"/>
<connect gate="G$1" pin="RESET" pad="8"/>
<connect gate="G$1" pin="SENSEA" pad="5"/>
<connect gate="G$1" pin="SENSEB" pad="17"/>
<connect gate="G$1" pin="SYNC" pad="15"/>
<connect gate="G$1" pin="VBB" pad="16"/>
<connect gate="G$1" pin="VDD" pad="6"/>
</connects>
<technologies>
<technology name="0"/>
<technology name="1"/>
<technology name="2"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM9044" prefix="IC">
<description>&lt;b&gt;Lambda Sensor Interface Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM9044.pdf</description>
<gates>
<gate name="G$1" symbol="LM9044"/>
</gates>
<devices>
<device name="V" package="PLCC20S">
<connects>
<connect gate="G$1" pin="+" pad="7"/>
<connect gate="G$1" pin="-" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="12"/>
<connect gate="G$1" pin="RF" pad="15"/>
<connect gate="G$1" pin="VCC" pad="17"/>
<connect gate="G$1" pin="VREF" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2937" prefix="IC">
<description>&lt;b&gt;LM2937-2.5, LM2937-3.3&lt;/b&gt; 400mA and 500mA Voltage Regulators&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM2937-2.5.pdf</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="TO263-3">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VI" pad="1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33215" prefix="IC">
<description>&lt;b&gt;Telefon Line Interface and Speakerphone Circuit&lt;/b&gt;&lt;p&gt;
Source: www.motorola.com .. MC33215.pdf</description>
<gates>
<gate name="G$1" symbol="MC33215"/>
</gates>
<devices>
<device name="FB" package="TQFP52">
<connects>
<connect gate="G$1" pin="!LSM" pad="19"/>
<connect gate="G$1" pin="!MUT" pad="13"/>
<connect gate="G$1" pin="!PRS" pad="17"/>
<connect gate="G$1" pin="AGC" pad="32"/>
<connect gate="G$1" pin="BM1" pad="8"/>
<connect gate="G$1" pin="BM2" pad="7"/>
<connect gate="G$1" pin="BVO" pad="38"/>
<connect gate="G$1" pin="GND" pad="31"/>
<connect gate="G$1" pin="GRX" pad="23"/>
<connect gate="G$1" pin="HM1" pad="5"/>
<connect gate="G$1" pin="HM2" pad="6"/>
<connect gate="G$1" pin="LSB" pad="42"/>
<connect gate="G$1" pin="LSF" pad="39"/>
<connect gate="G$1" pin="LSI" pad="36"/>
<connect gate="G$1" pin="LSO" pad="44"/>
<connect gate="G$1" pin="MFI" pad="4"/>
<connect gate="G$1" pin="NC@1" pad="14"/>
<connect gate="G$1" pin="NC@10" pad="52"/>
<connect gate="G$1" pin="NC@2" pad="15"/>
<connect gate="G$1" pin="NC@3" pad="20"/>
<connect gate="G$1" pin="NC@4" pad="25"/>
<connect gate="G$1" pin="NC@5" pad="26"/>
<connect gate="G$1" pin="NC@6" pad="40"/>
<connect gate="G$1" pin="NC@7" pad="41"/>
<connect gate="G$1" pin="NC@8" pad="46"/>
<connect gate="G$1" pin="NC@9" pad="51"/>
<connect gate="G$1" pin="PGD" pad="45"/>
<connect gate="G$1" pin="PPL" pad="37"/>
<connect gate="G$1" pin="RBN" pad="27"/>
<connect gate="G$1" pin="REF" pad="33"/>
<connect gate="G$1" pin="REG" pad="2"/>
<connect gate="G$1" pin="RLS" pad="30"/>
<connect gate="G$1" pin="RSA" pad="29"/>
<connect gate="G$1" pin="RSE" pad="28"/>
<connect gate="G$1" pin="RXI" pad="24"/>
<connect gate="G$1" pin="RXO" pad="22"/>
<connect gate="G$1" pin="RXS" pad="21"/>
<connect gate="G$1" pin="SLB" pad="1"/>
<connect gate="G$1" pin="SLP" pad="3"/>
<connect gate="G$1" pin="SPS" pad="16"/>
<connect gate="G$1" pin="SWD" pad="34"/>
<connect gate="G$1" pin="SWT" pad="18"/>
<connect gate="G$1" pin="TBN" pad="12"/>
<connect gate="G$1" pin="TSA" pad="10"/>
<connect gate="G$1" pin="TSE" pad="11"/>
<connect gate="G$1" pin="VCC" pad="47"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="VHF" pad="49"/>
<connect gate="G$1" pin="VLN" pad="48"/>
<connect gate="G$1" pin="VLS" pad="43"/>
<connect gate="G$1" pin="VMC" pad="50"/>
<connect gate="G$1" pin="VOL" pad="35"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM747H" prefix="IC">
<description>&lt;b&gt;Dual Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM747.pdf</description>
<gates>
<gate name="A" symbol="OPAMP+"/>
<gate name="B" symbol="OPAMP+"/>
<gate name="P" symbol="-V"/>
</gates>
<devices>
<device name="" package="H10C">
<connects>
<connect gate="A" pin="+IN" pad="4"/>
<connect gate="A" pin="-IN" pad="3"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="2"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OUT" pad="9"/>
<connect gate="B" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM747*" prefix="IC">
<description>&lt;b&gt;Dual Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM747.pdf</description>
<gates>
<gate name="A" symbol="OPAMP-OFF+V"/>
<gate name="B" symbol="OPAMP-OFF+V"/>
<gate name="P" symbol="-V1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="NULL1" pad="3"/>
<connect gate="A" pin="NULL2" pad="14"/>
<connect gate="A" pin="OUT" pad="12"/>
<connect gate="A" pin="V+" pad="13"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="NULL1" pad="5"/>
<connect gate="B" pin="NULL2" pad="8"/>
<connect gate="B" pin="OUT" pad="10"/>
<connect gate="B" pin="V+" pad="9"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="C"/>
<technology name="E"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDF8704*" prefix="IC">
<description>&lt;b&gt;8-bit high-speed analog-to-digital converter&lt;/b&gt; ADC&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/TDF8704_3.pdf</description>
<gates>
<gate name="G$1" symbol="TDF8704"/>
</gates>
<devices>
<device name="" package="SO24W">
<connects>
<connect gate="G$1" pin="!CE" pad="22"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="CLK" pad="16"/>
<connect gate="G$1" pin="D0" pad="2"/>
<connect gate="G$1" pin="D1" pad="1"/>
<connect gate="G$1" pin="D2" pad="24"/>
<connect gate="G$1" pin="D3" pad="23"/>
<connect gate="G$1" pin="D4" pad="15"/>
<connect gate="G$1" pin="D5" pad="14"/>
<connect gate="G$1" pin="D6" pad="13"/>
<connect gate="G$1" pin="D7" pad="12"/>
<connect gate="G$1" pin="DEC" pad="5"/>
<connect gate="G$1" pin="DGND" pad="17"/>
<connect gate="G$1" pin="O/UF" pad="11"/>
<connect gate="G$1" pin="OGND" pad="20"/>
<connect gate="G$1" pin="VCCA" pad="7"/>
<connect gate="G$1" pin="VCCD" pad="18"/>
<connect gate="G$1" pin="VCCO1" pad="19"/>
<connect gate="G$1" pin="VCCO2" pad="21"/>
<connect gate="G$1" pin="VI" pad="8"/>
<connect gate="G$1" pin="VRB" pad="4"/>
<connect gate="G$1" pin="VRT" pad="9"/>
</connects>
<technologies>
<technology name="T/2"/>
<technology name="T/4"/>
<technology name="T/5"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33269-SO8" prefix="IC">
<description>&lt;b&gt;Adjustable Output Low Dropout Voltage Regulator&lt;/b&gt; 800 mA&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC33269-D.PDF</description>
<gates>
<gate name="G$1" symbol="VREG-O4"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="GND/ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="OUT@1" pad="3"/>
<connect gate="G$1" pin="OUT@2" pad="6"/>
<connect gate="G$1" pin="OUT@3" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33269ST*" prefix="IC">
<description>&lt;b&gt;Adjustable Output Low Dropout Voltage Regulator&lt;/b&gt; 800 mA&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC33269-D.PDF</description>
<gates>
<gate name="G$1" symbol="VREG-O2"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND/ADJ" pad="1"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="OUT@1" pad="2"/>
</connects>
<technologies>
<technology name="-3.3T3"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33269?*" prefix="IC">
<description>&lt;b&gt;Adjustable Output Low Dropout Voltage Regulator&lt;/b&gt; 800 mA&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC33269-D.PDF</description>
<gates>
<gate name="G$1" symbol="317"/>
</gates>
<devices>
<device name="D" package="DPACK">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-12"/>
<technology name="-3.3"/>
<technology name="-5.0"/>
</technologies>
</device>
<device name="T" package="TO220V">
<connects>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-12"/>
<technology name="-3.3"/>
<technology name="-5.0"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TA8210A?*" prefix="IC">
<description>&lt;b&gt;20W BTL × 2ch Audio Power Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.semicon.toshiba.co.jp/td/en/ASSP/Audio_ICs/en_20050517_TA8210ALQ_datasheet.pdf</description>
<gates>
<gate name="G$1" symbol="TA8210"/>
</gates>
<devices>
<device name="L" package="HSIP17-P-2.00">
<connects>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="13"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="MUTE_SW" pad="1"/>
<connect gate="G$1" pin="NF1" pad="3"/>
<connect gate="G$1" pin="NF2" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="16"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="PRE-GND" pad="5"/>
<connect gate="G$1" pin="PRE-VCC" pad="9"/>
<connect gate="G$1" pin="RIPPLE" pad="8"/>
<connect gate="G$1" pin="STAND-BY_SW" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
<technology name="Q"/>
</technologies>
</device>
<device name="H" package="HZIP17-P-2.00">
<connects>
<connect gate="G$1" pin="GND@1" pad="14"/>
<connect gate="G$1" pin="GND@2" pad="13"/>
<connect gate="G$1" pin="IN1" pad="2"/>
<connect gate="G$1" pin="IN2" pad="7"/>
<connect gate="G$1" pin="MUTE_SW" pad="1"/>
<connect gate="G$1" pin="NF1" pad="3"/>
<connect gate="G$1" pin="NF2" pad="6"/>
<connect gate="G$1" pin="OUT1" pad="15"/>
<connect gate="G$1" pin="OUT2" pad="16"/>
<connect gate="G$1" pin="OUT3" pad="11"/>
<connect gate="G$1" pin="OUT4" pad="12"/>
<connect gate="G$1" pin="PRE-GND" pad="5"/>
<connect gate="G$1" pin="PRE-VCC" pad="9"/>
<connect gate="G$1" pin="RIPPLE" pad="8"/>
<connect gate="G$1" pin="STAND-BY_SW" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="10"/>
<connect gate="G$1" pin="VCC@2" pad="17"/>
</connects>
<technologies>
<technology name=""/>
<technology name="Q"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AN7161" prefix="IC">
<description>&lt;b&gt;BTL High Audio Power Amplifier&lt;/b&gt; AN7161NFP&lt;p&gt;
Source: http://www.steren.com.mx/diagramas/uploads/an7161.pdf</description>
<gates>
<gate name="G$1" symbol="AN7161"/>
</gates>
<devices>
<device name="" package="SIP-12">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="GND@OUT" pad="9"/>
<connect gate="G$1" pin="HEADPHONE" pad="1"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="IN-A" pad="2"/>
<connect gate="G$1" pin="IN-B" pad="5"/>
<connect gate="G$1" pin="OUT1" pad="10"/>
<connect gate="G$1" pin="OUT1A" pad="11"/>
<connect gate="G$1" pin="OUT2" pad="8"/>
<connect gate="G$1" pin="OUT2A" pad="7"/>
<connect gate="G$1" pin="RIPPLE" pad="6"/>
<connect gate="G$1" pin="VCC" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM340S" prefix="IC">
<description>&lt;b&gt;3-Terminal Positive Regulators&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM340.pdf</description>
<gates>
<gate name="G$1" symbol="LM340S"/>
</gates>
<devices>
<device name="" package="SOT223">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PA85*" prefix="IC">
<description>&lt;b&gt;HIGH VOLTAGE POWER OPERATIONAL AMPLIFIER&lt;/b&gt;&lt;p&gt;
Source: http://eportal.apexmicrotech.com .. mXvtzxx.pdf</description>
<gates>
<gate name="P" symbol="PA85"/>
</gates>
<devices>
<device name="" package="TO3-8">
<connects>
<connect gate="P" pin="+IN" pad="4"/>
<connect gate="P" pin="-IN" pad="5"/>
<connect gate="P" pin="CC" pad="8"/>
<connect gate="P" pin="OUT" pad="1"/>
<connect gate="P" pin="RC" pad="7"/>
<connect gate="P" pin="RCL" pad="2"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="6"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA*" prefix="IC">
<description>&lt;b&gt;Single Operational Amplifier&lt;/b&gt;&lt;p&gt;
Low Power, Single-Supply, Rail-To-Rail Operational Amplifier&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa2345.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="344"/>
<technology name="345"/>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="344"/>
<technology name="345"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2*" prefix="IC">
<description>&lt;b&gt;Dual Operational Amplifier&lt;/b&gt;&lt;p&gt;
Low Power, Single-Supply, Rail-To-Rail Operational Amplifier&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa2345.pdf&lt;br&gt;
http://focus.ti.com .. opa241.pdf&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/opa2134.pdf</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
<gate name="B" symbol="OPAMP"/>
</gates>
<devices>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="344"/>
<technology name="345"/>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="344"/>
</technologies>
</device>
<device name="E" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="344"/>
<technology name="345"/>
</technologies>
</device>
<device name="PA" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="134"/>
<technology name="241"/>
<technology name="251"/>
</technologies>
</device>
<device name="UA" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="8"/>
<connect gate="A" pin="V-" pad="4"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="134"/>
<technology name="241"/>
<technology name="251"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4*" prefix="IC">
<description>&lt;b&gt;Quad Operational Amplifier&lt;/b&gt;&lt;p&gt;
compatible with: TLC27L4&lt;p&gt;
Low Power, Single-Supply, Rail-To-Rail Operational Amplifier&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa2345.pdf&lt;br&gt;
http://focus.ti.com .. opa241.pdf&lt;br&gt;
http://focus.ti.com .. tlc27l4.pdf&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/opa2134.pdf&lt;br&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="344"/>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="344"/>
<technology name="345"/>
</technologies>
</device>
<device name="E" package="TSSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="344"/>
<technology name="345"/>
</technologies>
</device>
<device name="PA" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="134"/>
<technology name="241"/>
<technology name="251"/>
</technologies>
</device>
<device name="UA" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="134"/>
<technology name="241"/>
<technology name="251"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA*-SOT23" prefix="IC">
<description>&lt;b&gt;Single Operational Amplifier&lt;/b&gt;&lt;p&gt;
Low Power, Single-Supply, Rail-To-Rail Operational Amplifier&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa2345.pdf</description>
<gates>
<gate name="P" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="4"/>
<connect gate="P" pin="OUT" pad="1"/>
<connect gate="P" pin="V+" pad="5"/>
<connect gate="P" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="344N"/>
<technology name="345N"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PA241" prefix="IC">
<description>&lt;b&gt;High Voltage Power Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: eportal.apexmicrotech.com/mainsite/pdf/PA241u.pdf</description>
<gates>
<gate name="G$1" symbol="PA241"/>
</gates>
<devices>
<device name="DF" package="PSOP24">
<connects>
<connect gate="G$1" pin="+IN" pad="7"/>
<connect gate="G$1" pin="-IN" pad="5"/>
<connect gate="G$1" pin="C1" pad="17"/>
<connect gate="G$1" pin="C2" pad="19"/>
<connect gate="G$1" pin="ILIM" pad="15"/>
<connect gate="G$1" pin="OUT" pad="21"/>
<connect gate="G$1" pin="V+" pad="13"/>
<connect gate="G$1" pin="V-" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DW" package="SIP-10">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="C1" pad="9"/>
<connect gate="G$1" pin="C2" pad="8"/>
<connect gate="G$1" pin="ILIM" pad="7"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CE" package="TO3-8">
<connects>
<connect gate="G$1" pin="+IN" pad="6"/>
<connect gate="G$1" pin="-IN" pad="5"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="2"/>
<connect gate="G$1" pin="ILIM" pad="1"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="8"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA612A" prefix="IC">
<description>&lt;b&gt;Double-balanced mixer and oscillator&lt;/b&gt; NE612/SA612&lt;p&gt;
Source: www-eu2.semiconductors.philips.com/acrobat/datasheets/SA612A.pdf</description>
<gates>
<gate name="G$1" symbol="SA612A"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="IN-A" pad="1"/>
<connect gate="G$1" pin="IN-B" pad="2"/>
<connect gate="G$1" pin="OSC" pad="6"/>
<connect gate="G$1" pin="OSC'" pad="7"/>
<connect gate="G$1" pin="OUT-A" pad="4"/>
<connect gate="G$1" pin="OUT-B" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="IN-A" pad="1"/>
<connect gate="G$1" pin="IN-B" pad="2"/>
<connect gate="G$1" pin="OSC" pad="6"/>
<connect gate="G$1" pin="OSC'" pad="7"/>
<connect gate="G$1" pin="OUT-A" pad="4"/>
<connect gate="G$1" pin="OUT-B" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SLA7052MLF87" prefix="IC">
<description>&lt;b&gt;UNIPOLAR STEPPER-MOTOR TRANSLATOR/PWM DRIVER&lt;/b&gt;&lt;p&gt;
Source: http://www.allegromicro.com/datafile/97052.pdf</description>
<gates>
<gate name="G$1" symbol="SLA7052"/>
</gates>
<devices>
<device name="1" package="LF871">
<connects>
<connect gate="G$1" pin="!OUTA" pad="3"/>
<connect gate="G$1" pin="!OUTB" pad="16"/>
<connect gate="G$1" pin="CLOCK" pad="7"/>
<connect gate="G$1" pin="CW/CCW" pad="11"/>
<connect gate="G$1" pin="FULL/HALF" pad="12"/>
<connect gate="G$1" pin="GATEA" pad="4"/>
<connect gate="G$1" pin="GATEB" pad="15"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="OUTA" pad="1"/>
<connect gate="G$1" pin="OUTB" pad="18"/>
<connect gate="G$1" pin="REF" pad="9"/>
<connect gate="G$1" pin="SENSEA" pad="6"/>
<connect gate="G$1" pin="SENSEB" pad="13"/>
<connect gate="G$1" pin="SYNC" pad="8"/>
<connect gate="G$1" pin="VBB" pad="14"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2" package="LF872">
<connects>
<connect gate="G$1" pin="!OUTA" pad="3"/>
<connect gate="G$1" pin="!OUTB" pad="16"/>
<connect gate="G$1" pin="CLOCK" pad="7"/>
<connect gate="G$1" pin="CW/CCW" pad="11"/>
<connect gate="G$1" pin="FULL/HALF" pad="12"/>
<connect gate="G$1" pin="GATEA" pad="4"/>
<connect gate="G$1" pin="GATEB" pad="15"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="OUTA" pad="1"/>
<connect gate="G$1" pin="OUTB" pad="18"/>
<connect gate="G$1" pin="REF" pad="9"/>
<connect gate="G$1" pin="SENSEA" pad="6"/>
<connect gate="G$1" pin="SENSEB" pad="13"/>
<connect gate="G$1" pin="SYNC" pad="8"/>
<connect gate="G$1" pin="VBB" pad="14"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2574?-*" prefix="IC">
<description>&lt;b&gt;SIMPLE SWITCHER 0.5A Step-Down Voltage Regulator&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM2574.pdf</description>
<gates>
<gate name="G$1" symbol="LM2574"/>
</gates>
<devices>
<device name="HVN" package="DIL08">
<connects>
<connect gate="G$1" pin="!ON/OFF" pad="3"/>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="GND@PWR" pad="4"/>
<connect gate="G$1" pin="GNDSIG" pad="2"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="12"/>
<technology name="15"/>
<technology name="3.3"/>
<technology name="5.0"/>
<technology name="ADJ"/>
</technologies>
</device>
<device name="HVM" package="SO14W">
<connects>
<connect gate="G$1" pin="!ON/OFF" pad="5"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND@PWR" pad="6"/>
<connect gate="G$1" pin="GNDSIG" pad="4"/>
<connect gate="G$1" pin="IN" pad="10"/>
<connect gate="G$1" pin="OUT" pad="12"/>
</connects>
<technologies>
<technology name="12"/>
<technology name="15"/>
<technology name="3.3"/>
<technology name="5.0"/>
<technology name="ADJ"/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="!ON/OFF" pad="3"/>
<connect gate="G$1" pin="FB" pad="1"/>
<connect gate="G$1" pin="GND@PWR" pad="4"/>
<connect gate="G$1" pin="GNDSIG" pad="2"/>
<connect gate="G$1" pin="IN" pad="5"/>
<connect gate="G$1" pin="OUT" pad="7"/>
</connects>
<technologies>
<technology name="12"/>
<technology name="3.3"/>
<technology name="5.0"/>
<technology name="ADJ"/>
</technologies>
</device>
<device name="M" package="SO14W">
<connects>
<connect gate="G$1" pin="!ON/OFF" pad="5"/>
<connect gate="G$1" pin="FB" pad="3"/>
<connect gate="G$1" pin="GND@PWR" pad="6"/>
<connect gate="G$1" pin="GNDSIG" pad="4"/>
<connect gate="G$1" pin="IN" pad="10"/>
<connect gate="G$1" pin="OUT" pad="12"/>
</connects>
<technologies>
<technology name="12"/>
<technology name="15"/>
<technology name="3.3"/>
<technology name="5.0"/>
<technology name="ADJ"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ERA-*" prefix="IC">
<description>&lt;b&gt;MONOLITHIC AMPLIFIERS 50 Ohm BROADBAND DC to 8 GHz&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.mini-circuits.com/pdfs/ERA-3SM+.pdf"&gt;Datasheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ERA-3SM"/>
</gates>
<devices>
<device name="SM" package="WW">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="RFIN" pad="1"/>
<connect gate="G$1" pin="RFOUT/DCIN" pad="3"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="21"/>
<technology name="3"/>
<technology name="33"/>
<technology name="4"/>
<technology name="4X"/>
<technology name="5"/>
<technology name="50"/>
<technology name="51"/>
<technology name="5X"/>
<technology name="6"/>
<technology name="8"/>
</technologies>
</device>
<device name="" package="VV">
<connects>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="4"/>
<connect gate="G$1" pin="RFIN" pad="1"/>
<connect gate="G$1" pin="RFOUT/DCIN" pad="3"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
<technology name="3"/>
<technology name="4"/>
<technology name="5"/>
<technology name="6"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC14536B" prefix="IC">
<description>&lt;b&gt;Programmable Timer&lt;/b&gt;&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC14536B-D.PDF</description>
<gates>
<gate name="G$1" symbol="MC14536"/>
</gates>
<devices>
<device name="CP" package="DIL16">
<connects>
<connect gate="G$1" pin="8-BYPASS" pad="6"/>
<connect gate="G$1" pin="A" pad="9"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="11"/>
<connect gate="G$1" pin="CLOCK-INH" pad="7"/>
<connect gate="G$1" pin="D" pad="12"/>
<connect gate="G$1" pin="DECODE" pad="13"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="MONO-IN" pad="15"/>
<connect gate="G$1" pin="OSC-INH" pad="14"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SET" pad="1"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DW" package="SO16DW">
<connects>
<connect gate="G$1" pin="8-BYPASS" pad="6"/>
<connect gate="G$1" pin="A" pad="9"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="11"/>
<connect gate="G$1" pin="CLOCK-INH" pad="7"/>
<connect gate="G$1" pin="D" pad="12"/>
<connect gate="G$1" pin="DECODE" pad="13"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="MONO-IN" pad="15"/>
<connect gate="G$1" pin="OSC-INH" pad="14"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SET" pad="1"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F" package="SO16-F">
<connects>
<connect gate="G$1" pin="8-BYPASS" pad="6"/>
<connect gate="G$1" pin="A" pad="9"/>
<connect gate="G$1" pin="B" pad="10"/>
<connect gate="G$1" pin="C" pad="11"/>
<connect gate="G$1" pin="CLOCK-INH" pad="7"/>
<connect gate="G$1" pin="D" pad="12"/>
<connect gate="G$1" pin="DECODE" pad="13"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="MONO-IN" pad="15"/>
<connect gate="G$1" pin="OSC-INH" pad="14"/>
<connect gate="G$1" pin="OUT1" pad="4"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="RESET" pad="2"/>
<connect gate="G$1" pin="SET" pad="1"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF600T" prefix="IC">
<description>&lt;b&gt;Smart Com Radio Transceiver IC&lt;/b&gt;&lt;p&gt;
Source: http://www.rfsolutions.co.uk/acatalog/DS601-4.pdf</description>
<gates>
<gate name="G$1" symbol="RF600T"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="!CTS!/!LOOP" pad="2"/>
<connect gate="G$1" pin="!RTS" pad="4"/>
<connect gate="G$1" pin="!RXEN" pad="11"/>
<connect gate="G$1" pin="!TXEN!/RB" pad="10"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="12"/>
<connect gate="G$1" pin="IN2" pad="13"/>
<connect gate="G$1" pin="LEARN/LED" pad="3"/>
<connect gate="G$1" pin="MODE" pad="6"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="OUT1" pad="17"/>
<connect gate="G$1" pin="OUT2" pad="18"/>
<connect gate="G$1" pin="RXH" pad="8"/>
<connect gate="G$1" pin="RXR" pad="1"/>
<connect gate="G$1" pin="TXH" pad="7"/>
<connect gate="G$1" pin="TXR/HB" pad="9"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SO" package="SO18W300">
<connects>
<connect gate="G$1" pin="!CTS!/!LOOP" pad="2"/>
<connect gate="G$1" pin="!RTS" pad="4"/>
<connect gate="G$1" pin="!RXEN" pad="11"/>
<connect gate="G$1" pin="!TXEN!/RB" pad="10"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN1" pad="12"/>
<connect gate="G$1" pin="IN2" pad="13"/>
<connect gate="G$1" pin="LEARN/LED" pad="3"/>
<connect gate="G$1" pin="MODE" pad="6"/>
<connect gate="G$1" pin="OSC1" pad="16"/>
<connect gate="G$1" pin="OSC2" pad="15"/>
<connect gate="G$1" pin="OUT1" pad="17"/>
<connect gate="G$1" pin="OUT2" pad="18"/>
<connect gate="G$1" pin="RXH" pad="8"/>
<connect gate="G$1" pin="RXR" pad="1"/>
<connect gate="G$1" pin="TXH" pad="7"/>
<connect gate="G$1" pin="TXR/HB" pad="9"/>
<connect gate="G$1" pin="VCC" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1408" prefix="IC">
<description>&lt;b&gt;8-bit Multiplying D/A Converter&lt;/b&gt;&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC1408 DATASHEET.PDF</description>
<gates>
<gate name="G$1" symbol="MC1408"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="G$1" pin="A1" pad="5"/>
<connect gate="G$1" pin="A2" pad="6"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="8"/>
<connect gate="G$1" pin="A5" pad="9"/>
<connect gate="G$1" pin="A6" pad="10"/>
<connect gate="G$1" pin="A7" pad="11"/>
<connect gate="G$1" pin="A8" pad="12"/>
<connect gate="G$1" pin="COMPEN" pad="16"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IO" pad="4"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VEE" pad="3"/>
<connect gate="G$1" pin="VREF+" pad="14"/>
<connect gate="G$1" pin="VREF-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO16">
<connects>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A2" pad="10"/>
<connect gate="G$1" pin="A3" pad="11"/>
<connect gate="G$1" pin="A4" pad="12"/>
<connect gate="G$1" pin="A5" pad="13"/>
<connect gate="G$1" pin="A6" pad="14"/>
<connect gate="G$1" pin="A7" pad="15"/>
<connect gate="G$1" pin="A8" pad="16"/>
<connect gate="G$1" pin="COMPEN" pad="4"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="IO" pad="8"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VEE" pad="7"/>
<connect gate="G$1" pin="VREF+" pad="2"/>
<connect gate="G$1" pin="VREF-" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UDN2954W" prefix="IC">
<description>&lt;b&gt;FULL-BRIDGE PWM MOTOR DRIVER&lt;/b&gt;&lt;p&gt;
Allegro Microsystems&lt;br&gt;
Source: http://allegromicro.com/datafile/archive/2953.pdf</description>
<gates>
<gate name="G$1" symbol="UDN2954W"/>
</gates>
<devices>
<device name="" package="UDN2954W">
<connects>
<connect gate="G$1" pin="!OE" pad="9"/>
<connect gate="G$1" pin="A" pad="11"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="K" pad="3"/>
<connect gate="G$1" pin="OUTA" pad="10"/>
<connect gate="G$1" pin="OUTB" pad="2"/>
<connect gate="G$1" pin="PHASE" pad="8"/>
<connect gate="G$1" pin="RC" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="12"/>
<connect gate="G$1" pin="VBB" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VREF/!BREAK" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UDN2953B" prefix="IC">
<description>&lt;b&gt;FULL-BRIDGE PWM MOTOR DRIVER&lt;/b&gt;&lt;p&gt;
Allegro Microsystems&lt;br&gt;
Source: http://allegromicro.com/datafile/archive/2953.pdf</description>
<gates>
<gate name="G$1" symbol="UDN2953B"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="!OE" pad="8"/>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="12"/>
<connect gate="G$1" pin="GND@3" pad="13"/>
<connect gate="G$1" pin="K" pad="16"/>
<connect gate="G$1" pin="OUTA" pad="10"/>
<connect gate="G$1" pin="OUTB" pad="15"/>
<connect gate="G$1" pin="PHASE" pad="7"/>
<connect gate="G$1" pin="RC" pad="3"/>
<connect gate="G$1" pin="SENSE" pad="11"/>
<connect gate="G$1" pin="VBB" pad="9"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VREF/!BREAK" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A3977" prefix="IC">
<description>&lt;b&gt;MICROSTEPPING DMOS DRIVER WITH TRANSLATOR&lt;/b&gt;&lt;p&gt;
Source: http://allegromicro.com/datafile/3977.pdf</description>
<gates>
<gate name="G$1" symbol="A3977"/>
<gate name="P" symbol="A3977PWR"/>
</gates>
<devices>
<device name="SOCKED" package="PLCC-S44">
<connects>
<connect gate="G$1" pin="!ENABLE" pad="41"/>
<connect gate="G$1" pin="!RESET" pad="27"/>
<connect gate="G$1" pin="!SLEEP" pad="42"/>
<connect gate="G$1" pin="CP1" pad="37"/>
<connect gate="G$1" pin="CP2" pad="38"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HOME" pad="4"/>
<connect gate="G$1" pin="MS1" pad="20"/>
<connect gate="G$1" pin="MS2" pad="19"/>
<connect gate="G$1" pin="OUT1A" pad="6"/>
<connect gate="G$1" pin="OUT1B" pad="40"/>
<connect gate="G$1" pin="OUT2A" pad="18"/>
<connect gate="G$1" pin="OUT2B" pad="28"/>
<connect gate="G$1" pin="PFD" pad="9"/>
<connect gate="G$1" pin="RC1" pad="10"/>
<connect gate="G$1" pin="RC2" pad="15"/>
<connect gate="G$1" pin="REF" pad="14"/>
<connect gate="G$1" pin="SENSE1" pad="3"/>
<connect gate="G$1" pin="SENSE2" pad="21"/>
<connect gate="G$1" pin="SR" pad="26"/>
<connect gate="G$1" pin="STEP" pad="31"/>
<connect gate="G$1" pin="VBB1" pad="43"/>
<connect gate="G$1" pin="VBB2" pad="25"/>
<connect gate="G$1" pin="VCP" pad="36"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREG" pad="32"/>
<connect gate="P" pin="GND@1" pad="2"/>
<connect gate="P" pin="GND@10" pad="35"/>
<connect gate="P" pin="GND@11" pad="44"/>
<connect gate="P" pin="GND@2" pad="11"/>
<connect gate="P" pin="GND@3" pad="12"/>
<connect gate="P" pin="GND@4" pad="13"/>
<connect gate="P" pin="GND@5" pad="22"/>
<connect gate="P" pin="GND@6" pad="23"/>
<connect gate="P" pin="GND@7" pad="24"/>
<connect gate="P" pin="GND@8" pad="33"/>
<connect gate="P" pin="GND@9" pad="34"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="!ENABLE" pad="41"/>
<connect gate="G$1" pin="!RESET" pad="27"/>
<connect gate="G$1" pin="!SLEEP" pad="42"/>
<connect gate="G$1" pin="CP1" pad="37"/>
<connect gate="G$1" pin="CP2" pad="38"/>
<connect gate="G$1" pin="DIR" pad="5"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HOME" pad="4"/>
<connect gate="G$1" pin="MS1" pad="20"/>
<connect gate="G$1" pin="MS2" pad="19"/>
<connect gate="G$1" pin="OUT1A" pad="6"/>
<connect gate="G$1" pin="OUT1B" pad="40"/>
<connect gate="G$1" pin="OUT2A" pad="18"/>
<connect gate="G$1" pin="OUT2B" pad="28"/>
<connect gate="G$1" pin="PFD" pad="9"/>
<connect gate="G$1" pin="RC1" pad="10"/>
<connect gate="G$1" pin="RC2" pad="15"/>
<connect gate="G$1" pin="REF" pad="14"/>
<connect gate="G$1" pin="SENSE1" pad="3"/>
<connect gate="G$1" pin="SENSE2" pad="21"/>
<connect gate="G$1" pin="SR" pad="26"/>
<connect gate="G$1" pin="STEP" pad="31"/>
<connect gate="G$1" pin="VBB1" pad="43"/>
<connect gate="G$1" pin="VBB2" pad="25"/>
<connect gate="G$1" pin="VCP" pad="36"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREG" pad="32"/>
<connect gate="P" pin="GND@1" pad="2"/>
<connect gate="P" pin="GND@10" pad="35"/>
<connect gate="P" pin="GND@11" pad="44"/>
<connect gate="P" pin="GND@2" pad="11"/>
<connect gate="P" pin="GND@3" pad="12"/>
<connect gate="P" pin="GND@4" pad="13"/>
<connect gate="P" pin="GND@5" pad="22"/>
<connect gate="P" pin="GND@6" pad="23"/>
<connect gate="P" pin="GND@7" pad="24"/>
<connect gate="P" pin="GND@8" pad="33"/>
<connect gate="P" pin="GND@9" pad="34"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="A3979" prefix="IC">
<description>&lt;b&gt;Microstepping DMOS Driver with Translator&lt;/b&gt;&lt;p&gt;
Source: http://allegromicro.com/datafile/3979.pdf</description>
<gates>
<gate name="P" symbol="A3979"/>
</gates>
<devices>
<device name="" package="TSSOP28">
<connects>
<connect gate="P" pin="!ENABLE" pad="26"/>
<connect gate="P" pin="!RESET" pad="17"/>
<connect gate="P" pin="!SLEEP" pad="27"/>
<connect gate="P" pin="AGND" pad="7"/>
<connect gate="P" pin="CP1" pad="23"/>
<connect gate="P" pin="CP2" pad="24"/>
<connect gate="P" pin="DIR" pad="3"/>
<connect gate="P" pin="EXP" pad="EXP"/>
<connect gate="P" pin="HOME" pad="2"/>
<connect gate="P" pin="MS1" pad="13"/>
<connect gate="P" pin="MS2" pad="12"/>
<connect gate="P" pin="OUT1A" pad="4"/>
<connect gate="P" pin="OUT1B" pad="25"/>
<connect gate="P" pin="OUT2A" pad="11"/>
<connect gate="P" pin="OUT2B" pad="18"/>
<connect gate="P" pin="PFD" pad="5"/>
<connect gate="P" pin="PGND" pad="21"/>
<connect gate="P" pin="RC1" pad="6"/>
<connect gate="P" pin="RC2" pad="9"/>
<connect gate="P" pin="REF" pad="8"/>
<connect gate="P" pin="SENSE1" pad="1"/>
<connect gate="P" pin="SENSE2" pad="14"/>
<connect gate="P" pin="SR" pad="16"/>
<connect gate="P" pin="STEP" pad="19"/>
<connect gate="P" pin="VBB1" pad="28"/>
<connect gate="P" pin="VBB2" pad="15"/>
<connect gate="P" pin="VCP" pad="22"/>
<connect gate="P" pin="VDD" pad="10"/>
<connect gate="P" pin="VREG" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="U2400B" prefix="IC">
<description>&lt;b&gt;Charging of Batteries with Automatic Pre-Discharge&lt;/b&gt;&lt;p&gt;
Automatic recharging of NiCd / NiMH batteries.&lt;br&gt;
Source: http://www.elektronikpool.de/Sheets/U2400B.PDF</description>
<gates>
<gate name="G$1" symbol="U2400B"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="+VS" pad="8"/>
<connect gate="G$1" pin="0.5HZ" pad="16"/>
<connect gate="G$1" pin="CHARGE" pad="12"/>
<connect gate="G$1" pin="DISCHARGE" pad="10"/>
<connect gate="G$1" pin="FAILURE" pad="14"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="MODE" pad="15"/>
<connect gate="G$1" pin="OSC" pad="3"/>
<connect gate="G$1" pin="PWM" pad="2"/>
<connect gate="G$1" pin="STATUS" pad="9"/>
<connect gate="G$1" pin="SYNC" pad="1"/>
<connect gate="G$1" pin="TEMP" pad="5"/>
<connect gate="G$1" pin="TIME" pad="13"/>
<connect gate="G$1" pin="VMAX" pad="4"/>
<connect gate="G$1" pin="VMIN" pad="6"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-FP" package="SO16L">
<connects>
<connect gate="G$1" pin="+VS" pad="8"/>
<connect gate="G$1" pin="0.5HZ" pad="16"/>
<connect gate="G$1" pin="CHARGE" pad="12"/>
<connect gate="G$1" pin="DISCHARGE" pad="10"/>
<connect gate="G$1" pin="FAILURE" pad="14"/>
<connect gate="G$1" pin="GND" pad="11"/>
<connect gate="G$1" pin="MODE" pad="15"/>
<connect gate="G$1" pin="OSC" pad="3"/>
<connect gate="G$1" pin="PWM" pad="2"/>
<connect gate="G$1" pin="STATUS" pad="9"/>
<connect gate="G$1" pin="SYNC" pad="1"/>
<connect gate="G$1" pin="TEMP" pad="5"/>
<connect gate="G$1" pin="TIME" pad="13"/>
<connect gate="G$1" pin="VMAX" pad="4"/>
<connect gate="G$1" pin="VMIN" pad="6"/>
<connect gate="G$1" pin="VREF" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4995" prefix="IC">
<description>&lt;b&gt;1.3 Watt Audio Power Amplifier&lt;/b&gt; BOOMER Audio Power Amplifier Series&lt;p&gt;
Source: http://www.national.com .. LM4995.pdf</description>
<gates>
<gate name="G$1" symbol="LM4995"/>
</gates>
<devices>
<device name="" package="TMD09AAA">
<connects>
<connect gate="G$1" pin="!SHDOWN" pad="C1"/>
<connect gate="G$1" pin="BYPASS" pad="A1"/>
<connect gate="G$1" pin="GND" pad="A2"/>
<connect gate="G$1" pin="GND@1" pad="B2"/>
<connect gate="G$1" pin="IN+" pad="C3"/>
<connect gate="G$1" pin="IN-" pad="A3"/>
<connect gate="G$1" pin="VDD" pad="C2"/>
<connect gate="G$1" pin="VOL1-" pad="B3"/>
<connect gate="G$1" pin="VOL2+" pad="B1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC3*164" prefix="IC">
<description>&lt;b&gt;Micropower Undervoltage Sensing Circuits&lt;/b&gt;&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34164-D.PDF</description>
<gates>
<gate name="G$1" symbol="MC33164"/>
</gates>
<devices>
<device name="P" package="TO-226AA">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="2"/>
</connects>
<technologies>
<technology name="3"/>
<technology name="4"/>
</technologies>
</device>
<device name="SN" package="TSOP-5">
<connects>
<connect gate="G$1" pin="!RESET" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
</connects>
<technologies>
<technology name="4"/>
</technologies>
</device>
<device name="D" package="SOIC8">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="2"/>
</connects>
<technologies>
<technology name="3"/>
<technology name="4"/>
</technologies>
</device>
<device name="DM" package="MICRO8">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="2"/>
</connects>
<technologies>
<technology name="3"/>
<technology name="4"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA743" prefix="IC">
<description>&lt;b&gt;12V, 7MHz, CMOS, Rail-to-Rail I/O OP AMP&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/sbos201/sbos201.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2743" prefix="IC">
<description>&lt;b&gt;12V, 7MHz, CMOS, Rail-to-Rail I/O Dual OP AMP&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/sbos201/sbos201.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="EA" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PA" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="UA" package="SOIC8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4743" prefix="IC">
<description>&lt;b&gt;12V, 7MHz, CMOS, Rail-to-Rail I/O Quad OP AMP&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/sbos201/sbos201.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="UA" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EA" package="TSSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM321?*" prefix="IC">
<description>&lt;b&gt;Low Power Single Op Amp&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM321.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="MF" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="X"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3485" prefix="IC">
<description>&lt;b&gt;Hysteretic PFET Buck Controller&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM3485.pdf</description>
<gates>
<gate name="G$1" symbol="LM3485"/>
</gates>
<devices>
<device name="" package="MSOP08">
<connects>
<connect gate="G$1" pin="ADJ" pad="5"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="6"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="ISENSE" pad="1"/>
<connect gate="G$1" pin="PGATE" pad="7"/>
<connect gate="G$1" pin="VIN" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3966?-ADJ" prefix="IC">
<description>&lt;b&gt;3A Fast Ultra Low Dropout Linear Regulator&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LP/LP3963.pdf</description>
<gates>
<gate name="P" symbol="LP3966-ADJ"/>
</gates>
<devices>
<device name="ES" package="TO263-5">
<connects>
<connect gate="P" pin="!SD" pad="1"/>
<connect gate="P" pin="ADJ" pad="5"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="VIN" pad="2"/>
<connect gate="P" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3966?-*" prefix="IC">
<description>&lt;b&gt;3A Fast Ultra Low Dropout Linear Regulator&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LP/LP3963.pdf</description>
<gates>
<gate name="P" symbol="LP3966-SENSE"/>
</gates>
<devices>
<device name="ES" package="TO263-5">
<connects>
<connect gate="P" pin="!SD" pad="1"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="SENSE" pad="5"/>
<connect gate="P" pin="VIN" pad="2"/>
<connect gate="P" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="1.8"/>
<technology name="2.5"/>
<technology name="3.3"/>
<technology name="5.0"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP3963?*" prefix="IC">
<description>&lt;b&gt;3A Fast Ultra Low Dropout Linear Regulator&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LP/LP3963.pdf</description>
<gates>
<gate name="P" symbol="LP3963"/>
</gates>
<devices>
<device name="ES" package="TO263-5">
<connects>
<connect gate="P" pin="!ERROR" pad="5"/>
<connect gate="P" pin="!SD" pad="1"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="GND@1" pad="6"/>
<connect gate="P" pin="VIN" pad="2"/>
<connect gate="P" pin="VOUT" pad="4"/>
</connects>
<technologies>
<technology name="-1.8"/>
<technology name="-2.5"/>
<technology name="-3.3"/>
<technology name="-5.0"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT1166C" prefix="IC">
<description>&lt;b&gt;Power Output Stage Automatic Bias System&lt;/b&gt;&lt;p&gt;
Soource: http://www.linear.com</description>
<gates>
<gate name="G$1" symbol="LT1166"/>
</gates>
<devices>
<device name="N8" package="DIL08">
<connects>
<connect gate="G$1" pin="ILIM+" pad="7"/>
<connect gate="G$1" pin="ILIM-" pad="6"/>
<connect gate="G$1" pin="SENSE+" pad="8"/>
<connect gate="G$1" pin="SENSE-" pad="5"/>
<connect gate="G$1" pin="VBOTTOM" pad="4"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
<connect gate="G$1" pin="VTOP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S8" package="SO08">
<connects>
<connect gate="G$1" pin="ILIM+" pad="7"/>
<connect gate="G$1" pin="ILIM-" pad="6"/>
<connect gate="G$1" pin="SENSE+" pad="8"/>
<connect gate="G$1" pin="SENSE-" pad="5"/>
<connect gate="G$1" pin="VBOTTOM" pad="4"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
<connect gate="G$1" pin="VTOP" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL770*" prefix="IC">
<description>&lt;b&gt;SUPPLY VOLTAGE SUPERVISORS&lt;/b&gt; TL7700A Series&lt;p&gt;
Source: http://www.st.com/stonline/products/literature/ds/1528.pdf</description>
<gates>
<gate name="G$1" symbol="TL770X"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="!RESET" pad="5"/>
<connect gate="G$1" pin="!RESIN" pad="2"/>
<connect gate="G$1" pin="+VS" pad="8"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
</connects>
<technologies>
<technology name="02AC"/>
<technology name="02AI"/>
<technology name="05AC"/>
<technology name="05AI"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="!RESET" pad="5"/>
<connect gate="G$1" pin="!RESIN" pad="2"/>
<connect gate="G$1" pin="+VS" pad="8"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="REF" pad="1"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
</connects>
<technologies>
<technology name="02AC"/>
<technology name="02AI"/>
<technology name="05AC"/>
<technology name="05AI"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC27L*" prefix="IC">
<description>&lt;b&gt;LinCMOS(TM) PRECISION DUAL OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc27l2.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="PWR-VDDGND"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="GND" pad="4"/>
<connect gate="C" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="2AC"/>
<technology name="2AI"/>
<technology name="2BC"/>
<technology name="2BI"/>
<technology name="2C"/>
<technology name="2I"/>
<technology name="2M"/>
<technology name="7C"/>
<technology name="7I"/>
<technology name="7M"/>
</technologies>
</device>
<device name="D" package="SOIC8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="GND" pad="4"/>
<connect gate="C" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="2AC"/>
<technology name="2AI"/>
<technology name="2BC"/>
<technology name="2BI"/>
<technology name="2C"/>
<technology name="2I"/>
<technology name="2M"/>
<technology name="7C"/>
<technology name="7I"/>
<technology name="7M"/>
</technologies>
</device>
<device name="FK" package="PLCC20S">
<connects>
<connect gate="A" pin="+IN" pad="7"/>
<connect gate="A" pin="-IN" pad="5"/>
<connect gate="A" pin="OUT" pad="2"/>
<connect gate="B" pin="+IN" pad="12"/>
<connect gate="B" pin="-IN" pad="15"/>
<connect gate="B" pin="OUT" pad="17"/>
<connect gate="C" pin="GND" pad="10"/>
<connect gate="C" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name="2M"/>
<technology name="7M"/>
</technologies>
</device>
<device name="JG" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="GND" pad="4"/>
<connect gate="C" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="2M"/>
<technology name="7M"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM317LD" prefix="IC">
<description>&lt;b&gt;LOW CURRENT 1.2 TO 37V ADJUSTABLE VOLTAGE REGULATOR&lt;/b&gt;&lt;p&gt;
Source: http://pdf.alldatasheet.com</description>
<gates>
<gate name="G$1" symbol="LM317LD"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="VI" pad="1"/>
<connect gate="G$1" pin="VO" pad="2"/>
<connect gate="G$1" pin="VO@1" pad="3"/>
<connect gate="G$1" pin="VO@2" pad="6"/>
<connect gate="G$1" pin="VO@3" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3525M-L" prefix="IC">
<description>&lt;b&gt;Single Port USB Power Switch and Over-Current Protection&lt;/b&gt; LOW active&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM3525.pdf</description>
<gates>
<gate name="G$1" symbol="LM3525-L"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="!EN" pad="1"/>
<connect gate="G$1" pin="FLAG" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="7"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NC@1" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="OUT@1" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3525M-H" prefix="IC">
<description>&lt;b&gt;Single Port USB Power Switch and Over-Current Protection&lt;/b&gt; HIGH active&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM3525.pdf</description>
<gates>
<gate name="G$1" symbol="LM3525-H"/>
</gates>
<devices>
<device name="" package="SO08">
<connects>
<connect gate="G$1" pin="EN" pad="1"/>
<connect gate="G$1" pin="FLAG" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="IN" pad="7"/>
<connect gate="G$1" pin="NC" pad="4"/>
<connect gate="G$1" pin="NC@1" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="OUT@1" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM386?-*" prefix="IC">
<description>&lt;b&gt;Low Voltage Audio Power Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM386.pdf</description>
<gates>
<gate name="G$1" symbol="AMP_GND_GAIN_BYP"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BYPASS" pad="7"/>
<connect gate="G$1" pin="GAIN@1" pad="1"/>
<connect gate="G$1" pin="GAIN@2" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="3"/>
<technology name="4"/>
</technologies>
</device>
<device name="M" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BYPASS" pad="7"/>
<connect gate="G$1" pin="GAIN@1" pad="1"/>
<connect gate="G$1" pin="GAIN@2" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="1"/>
</technologies>
</device>
<device name="MM" package="MMSOP08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BYPASS" pad="7"/>
<connect gate="G$1" pin="GAIN@1" pad="1"/>
<connect gate="G$1" pin="GAIN@2" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="VS" pad="6"/>
</connects>
<technologies>
<technology name="1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LT10*" prefix="IC">
<description>&lt;b&gt;Low Noise, High Speed, Precision Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1154,C1009,C1026,P1212,D2204</description>
<gates>
<gate name="G$1" symbol="2CMP"/>
</gates>
<devices>
<device name="N8" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CMP1" pad="1"/>
<connect gate="G$1" pin="CMP2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="07AC"/>
<technology name="07C"/>
<technology name="07I"/>
<technology name="37AC"/>
<technology name="37C"/>
<technology name="37I"/>
</technologies>
</device>
<device name="S8" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CMP1" pad="1"/>
<connect gate="G$1" pin="CMP2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="07C"/>
<technology name="07I"/>
<technology name="37C"/>
<technology name="37I"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78L*" prefix="IC">
<description>&lt;b&gt;POSITOIV-VOLTAGE REGULATORS&lt;/b&gt;&lt;p&gt;
Output up to 100 mA&lt;br&gt;
Source: &lt;a href="http://focus.ti.com/lit/ds/symlink/ua78l05.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="78XX2GND"/>
</gates>
<devices>
<device name="F" package="SOT89">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="2@1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="1"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="08"/>
<technology name="09"/>
<technology name="10"/>
<technology name="12"/>
<technology name="15"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV321?*" prefix="IC">
<description>&lt;b&gt;General Purpose, Low Voltage, Rail-to-Rail Output Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/mpf/LM/LMV321.html&lt;br&gt;
http://www.national.com/dt/lmv_qual.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="M7" package="SC70-5L">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="X"/>
</technologies>
</device>
<device name="M5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="X"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV358?*" prefix="IC">
<description>Dual &lt;b&gt;General Purpose, Low Voltage, Rail-to-Rail Output Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/mpf/LM/LMV321.html&lt;br&gt;
http://www.national.com/dt/lmv_qual.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="M" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="X"/>
</technologies>
</device>
<device name="MM" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="X"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LMV324?*" prefix="IC">
<description>Quad &lt;b&gt;General Purpose, Low Voltage, Rail-to-Rail Output Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.national.com/mpf/LM/LMV321.html&lt;br&gt;
http://www.national.com/dt/lmv_qual.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="M" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="MZ" package="TSSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PA02" prefix="IC">
<description>&lt;b&gt;POWER OPERATIONAL AMPLIFIER&lt;/b&gt;&lt;p&gt;
SourcE: http://eportal.apexmicrotech.com/mainsite/pdf/pa02u.pdf&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="PA02"/>
</gates>
<devices>
<device name="SOCKET" package="0804MC">
<connects>
<connect gate="G$1" pin="+IN" pad="6"/>
<connect gate="G$1" pin="-IN" pad="5"/>
<connect gate="G$1" pin="OUT@1" pad="3"/>
<connect gate="G$1" pin="OUT@2" pad="4"/>
<connect gate="G$1" pin="RCL+" pad="1"/>
<connect gate="G$1" pin="RCL-" pad="8"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="TO3-8">
<connects>
<connect gate="G$1" pin="+IN" pad="6"/>
<connect gate="G$1" pin="-IN" pad="5"/>
<connect gate="G$1" pin="OUT@1" pad="3"/>
<connect gate="G$1" pin="OUT@2" pad="4"/>
<connect gate="G$1" pin="RCL+" pad="1"/>
<connect gate="G$1" pin="RCL-" pad="8"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA277" prefix="IC">
<description>&lt;b&gt;High Precision OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
REPLACES OP-07, OP-77, OP-177&lt;br&gt;
Source: opa277.pdf</description>
<gates>
<gate name="G$1" symbol="2CMP"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CMP1" pad="1"/>
<connect gate="G$1" pin="CMP2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CMP1" pad="1"/>
<connect gate="G$1" pin="CMP2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AIDRM" package="DFN8-4X4">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="CMP1" pad="1"/>
<connect gate="G$1" pin="CMP2" pad="8"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2277" prefix="IC">
<description>&lt;b&gt;High Precision OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
REPLACES OP-07, OP-77, OP-177&lt;br&gt;
Source: opa277.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="U" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AIDRM" package="DFN8-4X4">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4277" prefix="IC">
<description>&lt;b&gt;High Precision OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
REPLACES OP-07, OP-77, OP-177&lt;br&gt;
Source: opa277.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="U" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA728" prefix="IC">
<description>&lt;b&gt;Dual operational amplifier&lt;/b&gt;&lt;p&gt;
Source: ROHM BA728.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="F" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N" package="SIP8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GVA-84+" prefix="IC">
<description>&lt;b&gt;Monolithic Amplifier&lt;/b&gt; DC-6 GHz&lt;p&gt;
Source: GVA-84+.pdf</description>
<gates>
<gate name="G$1" symbol="GVA-84"/>
</gates>
<devices>
<device name="" package="SOT89">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="2"/>
<connect gate="G$1" pin="GND@2" pad="2@1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC34025" prefix="IC">
<description>&lt;b&gt;High Speed Double-Ended PWM Controller&lt;/b&gt;&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/MC34025-D.PDF</description>
<gates>
<gate name="G$1" symbol="MC34025"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="CLOCK" pad="4"/>
<connect gate="G$1" pin="CT" pad="6"/>
<connect gate="G$1" pin="ERROR" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LIM/SH-DOWN" pad="9"/>
<connect gate="G$1" pin="OUTA" pad="11"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="PGND" pad="12"/>
<connect gate="G$1" pin="RAMP" pad="7"/>
<connect gate="G$1" pin="RT" pad="5"/>
<connect gate="G$1" pin="SOFT-START" pad="8"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="G$1" pin="VREF" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DW" package="SO16W">
<connects>
<connect gate="G$1" pin="+IN" pad="2"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="CLOCK" pad="4"/>
<connect gate="G$1" pin="CT" pad="6"/>
<connect gate="G$1" pin="ERROR" pad="3"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="LIM/SH-DOWN" pad="9"/>
<connect gate="G$1" pin="OUTA" pad="11"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="PGND" pad="12"/>
<connect gate="G$1" pin="RAMP" pad="7"/>
<connect gate="G$1" pin="RT" pad="5"/>
<connect gate="G$1" pin="SOFT-START" pad="8"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VCC" pad="15"/>
<connect gate="G$1" pin="VREF" pad="16"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM5030" prefix="IC">
<description>&lt;b&gt;100V Push-Pull Current Mode PWM Controller&lt;/b&gt;&lt;p&gt;
Source: http://cache.national.com/ds/LM/LM5030.pdf</description>
<gates>
<gate name="G$1" symbol="LM5030"/>
</gates>
<devices>
<device name="MM" package="MSOP10">
<connects>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="SS" pad="10"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VFB" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SD" package="LLP10">
<connects>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT1" pad="5"/>
<connect gate="G$1" pin="OUT2" pad="6"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="SS" pad="10"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VFB" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2950" prefix="IC">
<description>&lt;b&gt;100 mA, Low Power Low Dropout Voltage Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/LP2950-D.PDF</description>
<gates>
<gate name="G$1" symbol="LP2950"/>
</gates>
<devices>
<device name="Z" package="TO92">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I" pad="3"/>
<connect gate="G$1" pin="O" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="" package="DPACK">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="I" pad="1"/>
<connect gate="G$1" pin="O" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2951" prefix="IC">
<description>&lt;b&gt;100 mA, Low Power Low Dropout Voltage Regulator&lt;/b&gt;&lt;p&gt;
Source: http://www.onsemi.com/pub/Collateral/LP2950-D.PDF</description>
<gates>
<gate name="G$1" symbol="LP2951"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="!ERROR" pad="5"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SH-DOWN" pad="3"/>
<connect gate="G$1" pin="VOTAB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DM" package="MICRO8">
<connects>
<connect gate="G$1" pin="!ERROR" pad="5"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SH-DOWN" pad="3"/>
<connect gate="G$1" pin="VOTAB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="N" package="DIL08">
<connects>
<connect gate="G$1" pin="!ERROR" pad="5"/>
<connect gate="G$1" pin="FB" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="8"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="SENSE" pad="2"/>
<connect gate="G$1" pin="SH-DOWN" pad="3"/>
<connect gate="G$1" pin="VOTAB" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UUC*806" prefix="IC">
<description>&lt;b&gt;LOW-POWER, DUAL-OUTPUT, CURRENT-MODE PWM CONTROLLER&lt;/b&gt;&lt;p&gt;
BiCMOS Version of UC3846 Family&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/ucc3806.pdf</description>
<gates>
<gate name="G$1" symbol="UUC1806"/>
</gates>
<devices>
<device name="D" package="SO16">
<connects>
<connect gate="G$1" pin="COMP" pad="7"/>
<connect gate="G$1" pin="CS+" pad="4"/>
<connect gate="G$1" pin="CS-" pad="3"/>
<connect gate="G$1" pin="CT" pad="8"/>
<connect gate="G$1" pin="CURLIM" pad="1"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INV" pad="6"/>
<connect gate="G$1" pin="NI" pad="5"/>
<connect gate="G$1" pin="OUTA" pad="11"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="SH-DOWN" pad="16"/>
<connect gate="G$1" pin="SYNC" pad="10"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name="2"/>
</technologies>
</device>
<device name="DW" package="SO16DW">
<connects>
<connect gate="G$1" pin="COMP" pad="7"/>
<connect gate="G$1" pin="CS+" pad="4"/>
<connect gate="G$1" pin="CS-" pad="3"/>
<connect gate="G$1" pin="CT" pad="8"/>
<connect gate="G$1" pin="CURLIM" pad="1"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INV" pad="6"/>
<connect gate="G$1" pin="NI" pad="5"/>
<connect gate="G$1" pin="OUTA" pad="11"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="SH-DOWN" pad="16"/>
<connect gate="G$1" pin="SYNC" pad="10"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name="2"/>
<technology name="3"/>
</technologies>
</device>
<device name="J" package="DIL16">
<connects>
<connect gate="G$1" pin="COMP" pad="7"/>
<connect gate="G$1" pin="CS+" pad="4"/>
<connect gate="G$1" pin="CS-" pad="3"/>
<connect gate="G$1" pin="CT" pad="8"/>
<connect gate="G$1" pin="CURLIM" pad="1"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INV" pad="6"/>
<connect gate="G$1" pin="NI" pad="5"/>
<connect gate="G$1" pin="OUTA" pad="11"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="SH-DOWN" pad="16"/>
<connect gate="G$1" pin="SYNC" pad="10"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name="1"/>
<technology name="2"/>
<technology name="3"/>
</technologies>
</device>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="COMP" pad="7"/>
<connect gate="G$1" pin="CS+" pad="4"/>
<connect gate="G$1" pin="CS-" pad="3"/>
<connect gate="G$1" pin="CT" pad="8"/>
<connect gate="G$1" pin="CURLIM" pad="1"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INV" pad="6"/>
<connect gate="G$1" pin="NI" pad="5"/>
<connect gate="G$1" pin="OUTA" pad="11"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="SH-DOWN" pad="16"/>
<connect gate="G$1" pin="SYNC" pad="10"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name="2"/>
<technology name="3"/>
</technologies>
</device>
<device name="Q" package="PLCC20S">
<connects>
<connect gate="G$1" pin="COMP" pad="9"/>
<connect gate="G$1" pin="CS+" pad="5"/>
<connect gate="G$1" pin="CS-" pad="4"/>
<connect gate="G$1" pin="CT" pad="10"/>
<connect gate="G$1" pin="CURLIM" pad="2"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="INV" pad="8"/>
<connect gate="G$1" pin="NI" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="14"/>
<connect gate="G$1" pin="OUTB" pad="18"/>
<connect gate="G$1" pin="RT" pad="12"/>
<connect gate="G$1" pin="SH-DOWN" pad="20"/>
<connect gate="G$1" pin="SYNC" pad="13"/>
<connect gate="G$1" pin="VC" pad="17"/>
<connect gate="G$1" pin="VIN" pad="19"/>
<connect gate="G$1" pin="VREF" pad="3"/>
</connects>
<technologies>
<technology name="2"/>
<technology name="3"/>
</technologies>
</device>
<device name="M" package="SSOP16">
<connects>
<connect gate="G$1" pin="COMP" pad="7"/>
<connect gate="G$1" pin="CS+" pad="4"/>
<connect gate="G$1" pin="CS-" pad="3"/>
<connect gate="G$1" pin="CT" pad="8"/>
<connect gate="G$1" pin="CURLIM" pad="1"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INV" pad="6"/>
<connect gate="G$1" pin="NI" pad="5"/>
<connect gate="G$1" pin="OUTA" pad="11"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="SH-DOWN" pad="16"/>
<connect gate="G$1" pin="SYNC" pad="10"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name="2"/>
</technologies>
</device>
<device name="PW" package="TSSOP16">
<connects>
<connect gate="G$1" pin="COMP" pad="7"/>
<connect gate="G$1" pin="CS+" pad="4"/>
<connect gate="G$1" pin="CS-" pad="3"/>
<connect gate="G$1" pin="CT" pad="8"/>
<connect gate="G$1" pin="CURLIM" pad="1"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="INV" pad="6"/>
<connect gate="G$1" pin="NI" pad="5"/>
<connect gate="G$1" pin="OUTA" pad="11"/>
<connect gate="G$1" pin="OUTB" pad="14"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="SH-DOWN" pad="16"/>
<connect gate="G$1" pin="SYNC" pad="10"/>
<connect gate="G$1" pin="VC" pad="13"/>
<connect gate="G$1" pin="VIN" pad="15"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM50" prefix="IC">
<description>&lt;b&gt;SOT-23 Single-Supply Centigrade Temperature Sensor&lt;/b&gt;&lt;p&gt;
Vout = (10mV/°C x Temp °C) +5mmmV&lt;br&gt;

Source: http://cache.national.com/ds/LM/LM50.pdf</description>
<gates>
<gate name="G$1" symbol="LM50"/>
</gates>
<devices>
<device name="" package="SOT23">
<connects>
<connect gate="G$1" pin="+VS" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8684" prefix="IC">
<description>&lt;b&gt;Quad Low Power, High Speed JFET Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/AD8682_8684.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RU" package="TSSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AD8682" prefix="IC">
<description>&lt;b&gt;Dual Low Power, High Speed JFET Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/AD8682_8684.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RM" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PA94" prefix="IC">
<description>&lt;b&gt;HIGH VOLTAGE POWER OPERATIONAL AMPLIFIER&lt;/b&gt; (900V)&lt;p&gt;
Source: www.apexmicrotech.com .. pa94u.pdf</description>
<gates>
<gate name="G1" symbol="PA94"/>
</gates>
<devices>
<device name="" package="SIP8-DQ">
<connects>
<connect gate="G1" pin="+IN" pad="2"/>
<connect gate="G1" pin="-IN" pad="1"/>
<connect gate="G1" pin="C1" pad="3"/>
<connect gate="G1" pin="C2" pad="4"/>
<connect gate="G1" pin="ILIM" pad="6"/>
<connect gate="G1" pin="OUT" pad="5"/>
<connect gate="G1" pin="V+" pad="8"/>
<connect gate="G1" pin="V-" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REF102" prefix="IC">
<description>&lt;b&gt;10V Precision Voltage Reference&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com .. ref102.pdf</description>
<gates>
<gate name="G$1" symbol="REF102"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="NOIS" pad="8"/>
<connect gate="G$1" pin="TRM" pad="5"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
<device name="U" package="0804MC">
<connects>
<connect gate="G$1" pin="COM" pad="4"/>
<connect gate="G$1" pin="NOIS" pad="8"/>
<connect gate="G$1" pin="TRM" pad="5"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="VO" pad="6"/>
</connects>
<technologies>
<technology name="A"/>
<technology name="B"/>
<technology name="C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BA612" prefix="IC">
<description>&lt;b&gt;5-channel high current driver&lt;/b&gt;&lt;p&gt;
Source: http://www.classiccmp.org/rtellason/chipdata/ba612.pdf</description>
<gates>
<gate name="A" symbol="INVERTER"/>
<gate name="B" symbol="INVERTER"/>
<gate name="C" symbol="INVERTER"/>
<gate name="D" symbol="INVERTER"/>
<gate name="E" symbol="INVERTER"/>
<gate name="P" symbol="GND"/>
</gates>
<devices>
<device name="" package="DIL14">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="13"/>
<connect gate="B" pin="I" pad="3"/>
<connect gate="B" pin="O" pad="12"/>
<connect gate="C" pin="I" pad="4"/>
<connect gate="C" pin="O" pad="11"/>
<connect gate="D" pin="I" pad="5"/>
<connect gate="D" pin="O" pad="10"/>
<connect gate="E" pin="I" pad="6"/>
<connect gate="E" pin="O" pad="9"/>
<connect gate="P" pin="O" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM336" prefix="IC">
<description>&lt;b&gt;2.5-V INTEGRATED REFERENCE CIRCUITS&lt;/b&gt;&lt;p&gt;
LM236&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/lm336-2.5.pdf</description>
<gates>
<gate name="G$1" symbol="LM336"/>
</gates>
<devices>
<device name="LP" package="TO92">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="ADJ" pad="1"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="A" pad="4"/>
<connect gate="G$1" pin="ADJ" pad="5"/>
<connect gate="G$1" pin="C" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP601" prefix="IC">
<description>&lt;b&gt;Single Op Amp&lt;/b&gt; 2.7V to 6.0V Single Supply CMOS&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="OT" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SN" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="2"/>
<connect gate="G$1" pin="V-" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP603" prefix="IC">
<description>&lt;b&gt;Dual Op Amp&lt;/b&gt; 2.7V to 6.0V Single Supply CMOS&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-CS"/>
</gates>
<devices>
<device name="CH" package="SOT23-6">
<connects>
<connect gate="G$1" pin="!CS" pad="5"/>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="6"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SN" package="SO08">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP602" prefix="IC">
<description>&lt;b&gt;Single Op Amp&lt;/b&gt; 2.7V to 6.0V Single Supply CMOS&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SN" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST" package="TSSOP8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP604" prefix="IC">
<description>&lt;b&gt;Quad Op Amp&lt;/b&gt; 2.7V to 6.0V Single Supply CMOS&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/21314g.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SL" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="ST" package="TSSOP14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC1350" prefix="IC">
<description>&lt;b&gt;Monolitic IF Amplifier&lt;/b&gt;&lt;p&gt;
Source: MOTOROLA .. MC1350.pdf</description>
<gates>
<gate name="G$1" symbol="MC1350"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="45/58MHZ" pad="3"/>
<connect gate="G$1" pin="AGC" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN+" pad="6"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT+" pad="8"/>
<connect gate="G$1" pin="OUT-" pad="1"/>
<connect gate="G$1" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="45/58MHZ" pad="3"/>
<connect gate="G$1" pin="AGC" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="IN+" pad="6"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT+" pad="8"/>
<connect gate="G$1" pin="OUT-" pad="1"/>
<connect gate="G$1" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TA7358P" prefix="IC">
<description>&lt;b&gt;FM FRONT-END&lt;/b&gt;&lt;p&gt;
Source: TOSHIBA TA7358P.pdf</description>
<gates>
<gate name="G$1" symbol="TA7358P"/>
</gates>
<devices>
<device name="" package="SIP9-P-2.54A">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="MIX-IN" pad="4"/>
<connect gate="G$1" pin="MIX-OUT" pad="6"/>
<connect gate="G$1" pin="OSC" pad="8"/>
<connect gate="G$1" pin="OSC-MONI" pad="7"/>
<connect gate="G$1" pin="RF-BY-PASS" pad="2"/>
<connect gate="G$1" pin="RF-IN" pad="1"/>
<connect gate="G$1" pin="RF-OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1703*" prefix="IC">
<description>&lt;b&gt;250 mA, 16V, Low Quiescent Current LDO Regulator&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/22049b.pdf</description>
<gates>
<gate name="G$1" symbol="MCP1703"/>
</gates>
<devices>
<device name="MB" package="SOT89">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="2"/>
<connect gate="G$1" pin="VI1" pad="2@1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="12"/>
<technology name="15"/>
<technology name="18"/>
<technology name="25"/>
<technology name="28"/>
<technology name="30"/>
<technology name="33"/>
<technology name="40"/>
<technology name="50"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1703" prefix="IC">
<description>&lt;b&gt;250 mA, 16V, Low Quiescent Current LDO Regulator&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/22049b.pdf</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="DB" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VI" pad="1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="CB" package="SOT23">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="3"/>
<connect gate="G$1" pin="VO" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UA78M*" prefix="IC">
<description>&lt;b&gt;POSITIVE-VOLTAGE REGULATORS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78m33.pdf</description>
<gates>
<gate name="G$1" symbol="78XX2GND"/>
</gates>
<devices>
<device name="DCY" package="SOT223">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="4"/>
<connect gate="G$1" pin="VI" pad="1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05"/>
<technology name="08"/>
<technology name="33"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2134" prefix="IC">
<description>&lt;b&gt;SoundPLUS (TM) High Performance AUDIO OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/sbos058/sbos058.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SOIC8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA4134" prefix="IC">
<description>&lt;b&gt;SoundPLUS (TM) High Performance AUDIO OPERATIONAL AMPLIFIERS&lt;p&gt;
Source: http://focus.ti.com/lit/ds/sbos058/sbos058.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA22*" prefix="IC">
<description>&lt;b&gt;High Precision, Low Noise OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa227.pdf</description>
<gates>
<gate name="P" symbol="OP+OFFSET"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="OFF1" pad="1"/>
<connect gate="P" pin="OFF2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="7"/>
<technology name="8"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="OFF1" pad="1"/>
<connect gate="P" pin="OFF2" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA222*" prefix="IC">
<description>&lt;b&gt;High Precision, Low Noise OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa227.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="7"/>
<technology name="8"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="7"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA422*" prefix="IC">
<description>&lt;b&gt;High Precision, Low Noise OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa227.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="7"/>
<technology name="8"/>
</technologies>
</device>
<device name="D" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name="7"/>
<technology name="8"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA5534" prefix="IC">
<description>&lt;b&gt;LOW-NOISE OPERATIONAL AMPLIFIER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ne5534.pdf</description>
<gates>
<gate name="A" symbol="2NUL2CMP"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="5"/>
<connect gate="A" pin="ON" pad="1"/>
<connect gate="A" pin="ON/CMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="CMP" pad="5"/>
<connect gate="A" pin="ON" pad="1"/>
<connect gate="A" pin="ON/CMP" pad="8"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA725" prefix="IC">
<description>&lt;b&gt;Very Low Noise, High-Speed, 12V CMOS Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa725.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2725" prefix="IC">
<description>&lt;b&gt;Very Low Noise, High-Speed, 12V CMOS Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa725.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DGK" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA726" prefix="IC">
<description>&lt;b&gt;Very Low Noise, High-Speed, 12V CMOS Operational Amplifier&lt;/b&gt; with Shutdown&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa725.pdf</description>
<gates>
<gate name="P" symbol="OPA726"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="DGND" pad="1"/>
<connect gate="P" pin="EN" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DGK" package="MSOP08">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="DGND" pad="1"/>
<connect gate="P" pin="EN" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2726" prefix="IC">
<description>&lt;b&gt;Very Low Noise, High-Speed, 12V CMOS Operational Amplifier&lt;/b&gt; with Shutdown&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/opa725.pdf</description>
<gates>
<gate name="P" symbol="OPA2726"/>
</gates>
<devices>
<device name="" package="MSOP10">
<connects>
<connect gate="P" pin="+INA" pad="3"/>
<connect gate="P" pin="+INB" pad="7"/>
<connect gate="P" pin="-INA" pad="2"/>
<connect gate="P" pin="-INB" pad="8"/>
<connect gate="P" pin="DGND" pad="5"/>
<connect gate="P" pin="EN" pad="6"/>
<connect gate="P" pin="OUTA" pad="1"/>
<connect gate="P" pin="OUTB" pad="9"/>
<connect gate="P" pin="V+" pad="10"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM*18" prefix="IC">
<description>&lt;b&gt;FAST GENERAL-PURPOSE OPERATIONAL AMPLIFIER&lt;/b&gt;&lt;p&gt;
Sourde: http://focus.ti.com/lit/ds/slos063b/slos063b.pdf</description>
<gates>
<gate name="P" symbol="OPAMP-BAL-CMP"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="BAL1" pad="1"/>
<connect gate="P" pin="BAL2" pad="5"/>
<connect gate="P" pin="COMP" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="3"/>
</technologies>
</device>
<device name="D" package="SOIC8">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="BAL1" pad="1"/>
<connect gate="P" pin="BAL2" pad="5"/>
<connect gate="P" pin="COMP" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="3"/>
</technologies>
</device>
<device name="PS" package="PS_R-PDSO-G8">
<connects>
<connect gate="P" pin="+IN" pad="3"/>
<connect gate="P" pin="-IN" pad="2"/>
<connect gate="P" pin="BAL1" pad="1"/>
<connect gate="P" pin="BAL2" pad="5"/>
<connect gate="P" pin="COMP" pad="8"/>
<connect gate="P" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="7"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name="3"/>
</technologies>
</device>
<device name="FK" package="LCCC20">
<connects>
<connect gate="P" pin="+IN" pad="7"/>
<connect gate="P" pin="-IN" pad="5"/>
<connect gate="P" pin="BAL1" pad="2"/>
<connect gate="P" pin="BAL2" pad="12"/>
<connect gate="P" pin="COMP" pad="20"/>
<connect gate="P" pin="OUT" pad="15"/>
<connect gate="P" pin="V+" pad="17"/>
<connect gate="P" pin="V-" pad="10"/>
</connects>
<technologies>
<technology name="1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL331" prefix="IC">
<description>&lt;b&gt;SINGLE DIFFERENTIAL COMPARATOR&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/tl331-q1.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="OPAMP+GN"/>
</gates>
<devices>
<device name="" package="DBV-R-PDSO-G5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HA5024" prefix="IC">
<description>&lt;b&gt;Quad 125MHz Video Current Feedback Amplifier with Disable&lt;/b&gt;&lt;p&gt;
Source: http://www.intersil.com/data/fn/fn3550.pdf</description>
<gates>
<gate name="A" symbol="OPAMP_CS"/>
<gate name="B" symbol="OPAMP_CS"/>
<gate name="C" symbol="OPAMP_CS"/>
<gate name="D" symbol="OPAMP_CS"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="A" pin="!CS" pad="4"/>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="!CS" pad="7"/>
<connect gate="B" pin="+IN" pad="8"/>
<connect gate="B" pin="-IN" pad="9"/>
<connect gate="B" pin="OUT" pad="10"/>
<connect gate="C" pin="!CS" pad="14"/>
<connect gate="C" pin="+IN" pad="13"/>
<connect gate="C" pin="-IN" pad="12"/>
<connect gate="C" pin="OUT" pad="11"/>
<connect gate="D" pin="!CS" pad="17"/>
<connect gate="D" pin="+IN" pad="18"/>
<connect gate="D" pin="-IN" pad="19"/>
<connect gate="D" pin="OUT" pad="20"/>
<connect gate="P" pin="V+" pad="6"/>
<connect gate="P" pin="V-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="B" package="SO20W">
<connects>
<connect gate="A" pin="!CS" pad="4"/>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="!CS" pad="7"/>
<connect gate="B" pin="+IN" pad="8"/>
<connect gate="B" pin="-IN" pad="9"/>
<connect gate="B" pin="OUT" pad="10"/>
<connect gate="C" pin="!CS" pad="14"/>
<connect gate="C" pin="+IN" pad="13"/>
<connect gate="C" pin="-IN" pad="12"/>
<connect gate="C" pin="OUT" pad="11"/>
<connect gate="D" pin="!CS" pad="17"/>
<connect gate="D" pin="+IN" pad="18"/>
<connect gate="D" pin="-IN" pad="19"/>
<connect gate="D" pin="OUT" pad="20"/>
<connect gate="P" pin="V+" pad="6"/>
<connect gate="P" pin="V-" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP183">
<description>&lt;b&gt;5 MHz Single-Supply Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/OP183.pdf</description>
<gates>
<gate name="S" symbol="OP+OFFSET"/>
</gates>
<devices>
<device name="S" package="SO08">
<connects>
<connect gate="S" pin="+IN" pad="3"/>
<connect gate="S" pin="-IN" pad="2"/>
<connect gate="S" pin="OFF1" pad="1"/>
<connect gate="S" pin="OFF2" pad="5"/>
<connect gate="S" pin="OUT" pad="6"/>
<connect gate="S" pin="V+" pad="7"/>
<connect gate="S" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP249" prefix="IC">
<description>&lt;b&gt;Dual, Precision JFET High Speed Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/OP249.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="N" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="1"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="OUT" pad="7"/>
<connect gate="B" pin="+IN" pad="3"/>
<connect gate="B" pin="-IN" pad="4"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="P" pin="V+" pad="6"/>
<connect gate="P" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP270" prefix="IC">
<description>&lt;b&gt;Dual Very Low Noise Precision Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/OP270.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO16">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="16"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OUT" pad="10"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP275" prefix="IC">
<description>&lt;b&gt;Dual Very Low Noise Precision Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/OP270.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO16">
<connects>
<connect gate="A" pin="+IN" pad="2"/>
<connect gate="A" pin="-IN" pad="1"/>
<connect gate="A" pin="OUT" pad="16"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="7"/>
<connect gate="B" pin="OUT" pad="10"/>
<connect gate="P" pin="V+" pad="13"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP97" prefix="IC">
<description>&lt;b&gt;Low Power, High Precision Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/OP97.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP-BAL-CMP"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BAL1" pad="1"/>
<connect gate="G$1" pin="BAL2" pad="8"/>
<connect gate="G$1" pin="COMP" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="BAL1" pad="1"/>
<connect gate="G$1" pin="BAL2" pad="8"/>
<connect gate="G$1" pin="COMP" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA333" prefix="IC">
<description>&lt;b&gt;1.8V, microPOWER CMOS OPERATIONAL AMPLIFIERS Zerø-Drift Series&lt;/b&gt;&lt;p&gt;
Source: Texas Instruments (Burr-Brown) .. U11 opa333 Operational Amp.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="DCK" package="SC70-5L">
<connects>
<connect gate="G$1" pin="+IN" pad="1"/>
<connect gate="G$1" pin="-IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="V+" pad="5"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPA2333" prefix="IC">
<description>&lt;b&gt;DUAL 1.8V, microPOWER CMOS OPERATIONAL AMPLIFIERS Zerø-Drift Series&lt;/b&gt;&lt;p&gt;
Source: Texas Instruments (Burr-Brown) .. U11 opa333 Operational Amp.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DRB" package="DFN8-4X4">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DGK" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC78M" prefix="IC">
<description>&lt;b&gt;500 mA Positive Voltage Regulators&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.onsemi.com/pub_link/Collateral/MC78M00-D.PDF"&gt;Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="DPACK_3">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VI" pad="1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05ABDT"/>
<technology name="05ACDTG"/>
<technology name="05BDTG"/>
<technology name="05BDTRKG"/>
<technology name="05CDTG"/>
<technology name="06CDTG"/>
<technology name="06CDTRKG"/>
<technology name="08ABDTG"/>
<technology name="08ACDTG"/>
<technology name="08BDTG"/>
<technology name="08CDTG"/>
<technology name="09BDTG"/>
<technology name="09BDTRKG"/>
<technology name="09CDTG"/>
<technology name="12BDTG"/>
<technology name="12CDTG"/>
<technology name="12CDTRKG"/>
<technology name="12CDTT5G"/>
<technology name="15ABDTG"/>
<technology name="15ABDTRKG"/>
<technology name="15ACDTG"/>
<technology name="15CDTG"/>
<technology name="15CDTRKG"/>
<technology name="18CDTG"/>
</technologies>
</device>
<device name="T" package="TO220V">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VI" pad="1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05AB"/>
<technology name="05ACT"/>
<technology name="05B"/>
<technology name="05C"/>
<technology name="06B"/>
<technology name="06C"/>
<technology name="08AB"/>
<technology name="08AC"/>
<technology name="08B"/>
<technology name="08C"/>
<technology name="09B"/>
<technology name="09C"/>
<technology name="12AB"/>
<technology name="12AC"/>
<technology name="12B"/>
<technology name="12C"/>
<technology name="15AB"/>
<technology name="15AC"/>
<technology name="15B"/>
<technology name="15C"/>
<technology name="18B"/>
<technology name="18C"/>
<technology name="20B"/>
<technology name="20C"/>
<technology name="24B"/>
<technology name="24C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCV78M" prefix="IC">
<description>&lt;b&gt;500 mA Positive Voltage Regulators&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.onsemi.com/pub_link/Collateral/MC78M00-D.PDF"&gt;Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="78XX"/>
</gates>
<devices>
<device name="" package="DPACK_3">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VI" pad="1"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05BDTRKG"/>
<technology name="08BDTRKG"/>
<technology name="12BDTRKG"/>
<technology name="15BDTG"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC79M" prefix="IC">
<description>&lt;b&gt;500 mA Negative Voltage Regulators&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.onsemi.com/pub_link/Collateral/MC79M00-D.PDF"&gt;Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="79XX"/>
</gates>
<devices>
<device name="" package="DPACK_3">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="4"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05BDTG"/>
<technology name="05BDTRKG"/>
<technology name="05CDTG"/>
<technology name="05CDTRKG"/>
<technology name="08CDTG"/>
<technology name="08CDTRKG"/>
<technology name="12BDTG"/>
<technology name="12BDTRKG"/>
<technology name="12CDTG"/>
<technology name="15BDTG"/>
<technology name="15BDTRKG"/>
<technology name="15CDTG"/>
<technology name="15CDTRKG"/>
</technologies>
</device>
<device name="T" package="TO220V">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VI" pad="2"/>
<connect gate="G$1" pin="VO" pad="3"/>
</connects>
<technologies>
<technology name="05B"/>
<technology name="05C"/>
<technology name="08B"/>
<technology name="08C"/>
<technology name="12B"/>
<technology name="12C"/>
<technology name="15B"/>
<technology name="15C"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP1177" prefix="IC">
<description>&lt;b&gt;Precision Low Noise, Low Input Bias Current Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: OP1177_2177_4177.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="RM" package="MSOP08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R" package="SOIC8">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP1277" prefix="IC">
<description>&lt;b&gt;Precision Low Noise, Low Input Bias Current Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: OP1177_2177_4177.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="RM" package="MSOP08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="R" package="SOIC8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP1477" prefix="IC">
<description>&lt;b&gt;Precision Low Noise, Low Input Bias Current Operational Amplifiers&lt;/b&gt;&lt;p&gt;
Source: OP1177_2177_4177.pdf</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="R" package="SO14">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RU" package="TSSOP14-RU">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="C" pin="+IN" pad="10"/>
<connect gate="C" pin="-IN" pad="9"/>
<connect gate="C" pin="OUT" pad="8"/>
<connect gate="D" pin="+IN" pad="12"/>
<connect gate="D" pin="-IN" pad="13"/>
<connect gate="D" pin="OUT" pad="14"/>
<connect gate="P" pin="V+" pad="4"/>
<connect gate="P" pin="V-" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TS931?*" prefix="IC">
<description>&lt;b&gt;Output rail-to-rail micropower operational amplifiers&lt;/b&gt;&lt;p&gt;
Source: http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/CD00001973.pdf</description>
<gates>
<gate name="A" symbol="OPAMP+-"/>
</gates>
<devices>
<device name="ILT" package="SOT23-5">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="4"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="A" pin="V+" pad="5"/>
<connect gate="A" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
</technologies>
</device>
<device name="IDT" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="A" pin="V+" pad="7"/>
<connect gate="A" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
<technology name="A"/>
<technology name="B"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
