<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Low Power Radio Solutions Ltd&lt;/b&gt;&lt;p&gt;
The easyRadio (ER) ERx00TS Transmitter, ERx00RS Receiver and ERx00TRS transceiver incorporate 'easyRadio' technology to provide high performance, simple to use radio devices that can transfer data over a range of up to 250 metres Line Of Sight (LOS).  ER modules are available in two frequency versions: ER400 series (433-434MHz) &amp; ER900 series (869.85MHz &amp; 902-928MHz). &lt;br&gt;
http://www.lprs.co.uk</description>
<packages>
<package name="SIL9">
<description>&lt;b&gt;Single In ine 9 leads&lt;/b&gt; ER Receiver&lt;p&gt;
Source: http://www.lprs.co.uk/pdf_directory/2386mylprs1132229147er-datasheet-2.3-sept-05.pdf</description>
</package>
<package name="SIL5">
<description>&lt;b&gt;Single In ine 5 leads&lt;/b&gt; ER Transmitter&lt;p&gt;
Source: http://www.lprs.co.uk/pdf_directory/2386mylprs1132229147er-datasheet-2.3-sept-05.pdf</description>
</package>
</packages>
<symbols>
<symbol name="ER-TRANSMITTER">
<pin name="ANT" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="TXD" direction="in"/>
<pin name="RFGND" direction="in"/>
</symbol>
<symbol name="ER-RECEIVER">
<pin name="ANT" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="SDI"/>
<pin name="RFGND" direction="in"/>
<pin name="RSSI" direction="out"/>
<pin name="SDO" direction="out"/>
<pin name="BSY"/>
<pin name="RDY"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ER*00TS-02" prefix="IC">
<description>&lt;b&gt;Easy-Radio '02' (2nd Generation Modules)&lt;/b&gt; Transmitter&lt;p&gt;
Source: http://www.lprs.co.uk/pdf_directory/2386mylprs1132229147er-datasheet-2.3-sept-05.pdf</description>
<gates>
<gate name="G$1" symbol="ER-TRANSMITTER"/>
</gates>
<devices>
<device name="" package="SIL5">
<connects>
<connect gate="G$1" pin="ANT" pad="2"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RFGND" pad="1"/>
<connect gate="G$1" pin="TXD" pad="5"/>
<connect gate="G$1" pin="VCC" pad="3"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ER400TS"/>
<attribute name="OC_FARNELL" value="5096510"/>
<attribute name="OC_NEWARK" value="13J9294"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ER900TS"/>
<attribute name="OC_FARNELL" value="5096534"/>
<attribute name="OC_NEWARK" value="13J9299"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ER*00RS-02" prefix="IC">
<description>&lt;b&gt;Easy-Radio '02' (2nd Generation Modules)&lt;/b&gt; Receiver&lt;p&gt;
Source: http://www.lprs.co.uk/pdf_directory/2386mylprs1132229147er-datasheet-2.3-sept-05.pdf</description>
<gates>
<gate name="G$1" symbol="ER-RECEIVER"/>
</gates>
<devices>
<device name="" package="SIL9">
<connects>
<connect gate="G$1" pin="ANT" pad="2"/>
<connect gate="G$1" pin="BSY" pad="4"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="RDY" pad="7"/>
<connect gate="G$1" pin="RFGND" pad="1"/>
<connect gate="G$1" pin="RSSI" pad="3"/>
<connect gate="G$1" pin="SDI" pad="6"/>
<connect gate="G$1" pin="SDO" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ER400RS"/>
<attribute name="OC_FARNELL" value="5096522"/>
<attribute name="OC_NEWARK" value="13J9292"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ER900RS"/>
<attribute name="OC_FARNELL" value="5096546"/>
<attribute name="OC_NEWARK" value="13J9297"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ER*00RTS-02" prefix="IC">
<description>&lt;b&gt;Easy-Radio '02' (2nd Generation Modules)&lt;/b&gt; Transceiver&lt;p&gt;
Source: http://www.lprs.co.uk/pdf_directory/2386mylprs1132229147er-datasheet-2.3-sept-05.pdf</description>
<gates>
<gate name="G$1" symbol="ER-RECEIVER"/>
</gates>
<devices>
<device name="" package="SIL9">
<connects>
<connect gate="G$1" pin="ANT" pad="1"/>
<connect gate="G$1" pin="BSY" pad="4"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="RDY" pad="7"/>
<connect gate="G$1" pin="RFGND" pad="2"/>
<connect gate="G$1" pin="RSSI" pad="3"/>
<connect gate="G$1" pin="SDI" pad="6"/>
<connect gate="G$1" pin="SDO" pad="5"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ER400RS"/>
<attribute name="OC_FARNELL" value="5096522"/>
<attribute name="OC_NEWARK" value="13J9292"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ER900RS"/>
<attribute name="OC_FARNELL" value="5096546"/>
<attribute name="OC_NEWARK" value="13J9297"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
