<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;LSI Computer Systems, Inc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL48">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TSSOP48">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 48&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/TSSOP_OD.pdf</description>
</package>
<package name="TSSOP38">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 38&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/TSSOP_OD.pdf</description>
</package>
<package name="TSSOP28">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 28&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/TSSOP_OD.pdf</description>
</package>
<package name="TSSOP24">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 24&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/TSSOP_OD.pdf</description>
</package>
<package name="TSSOP20">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 20&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/TSSOP_OD.pdf</description>
</package>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/TSSOP_OD.pdf</description>
</package>
<package name="SOIC28L">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt; 17.9 x 10.3 &lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/SOIC%20Outline%20Dwgs.pdf</description>
</package>
<package name="SOIC24L">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt; 15.4 x 10.3 &lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/SOIC%20Outline%20Dwgs.pdf</description>
</package>
<package name="SOIC20L">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt; 12.8 x 10.3 &lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/SOIC%20Outline%20Dwgs.pdf</description>
</package>
<package name="SOIC18L">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt; 11.55 x 10.3 &lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/SOIC%20Outline%20Dwgs.pdf</description>
</package>
<package name="SOIC16LWB">
<description>&lt;b&gt;SMALL OUTLINE PACKAGE&lt;/b&gt; 10.3 x 10.3 &lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Drawings/SOIC%20Outline%20Dwgs.pdf</description>
</package>
</packages>
<symbols>
<symbol name="LS7766DH">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="DB8" direction="hiz"/>
<pin name="DB9" direction="hiz"/>
<pin name="DB10" direction="hiz"/>
<pin name="DB11" direction="hiz"/>
<pin name="DB12" direction="hiz"/>
<pin name="DB13" direction="hiz"/>
<pin name="DB14" direction="hiz"/>
<pin name="DB15" direction="hiz"/>
<pin name="RS0" direction="in"/>
<pin name="RS1" direction="in"/>
<pin name="RS2" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="PCKO" direction="out"/>
<pin name="PCKI" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!IO16" direction="in"/>
<pin name="X1A" direction="in"/>
<pin name="X1B" direction="in"/>
<pin name="!X1INDX" direction="in"/>
<pin name="X1FLGA" direction="out"/>
<pin name="X1FLGB" direction="out"/>
<pin name="X1CKO" direction="out"/>
<pin name="!X0!_X1" direction="out"/>
<pin name="X0CKO" direction="out"/>
<pin name="X0A" direction="in"/>
<pin name="X0B" direction="in"/>
<pin name="X0FLGA" direction="out"/>
<pin name="X0FLGB" direction="out"/>
<pin name="!X0INDX" direction="in"/>
<pin name="VSS@2" direction="pwr"/>
</symbol>
<symbol name="LS7766DO">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="RS0" direction="in"/>
<pin name="RS1" direction="in"/>
<pin name="RS2" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="PCKI" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="X1A" direction="in"/>
<pin name="X1B" direction="in"/>
<pin name="!X1INDX" direction="in"/>
<pin name="X1FLGA" direction="out"/>
<pin name="X1FLGB" direction="out"/>
<pin name="!X0!_X1" direction="out"/>
<pin name="X0A" direction="in"/>
<pin name="X0B" direction="in"/>
<pin name="X0FLGA" direction="out"/>
<pin name="X0FLGB" direction="out"/>
<pin name="!X0INDX" direction="in"/>
</symbol>
<symbol name="LS7766SH">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="DB8" direction="hiz"/>
<pin name="DB9" direction="hiz"/>
<pin name="DB10" direction="hiz"/>
<pin name="DB11" direction="hiz"/>
<pin name="DB12" direction="hiz"/>
<pin name="DB13" direction="hiz"/>
<pin name="DB14" direction="hiz"/>
<pin name="DB15" direction="hiz"/>
<pin name="RS0" direction="in"/>
<pin name="RS1" direction="in"/>
<pin name="RS2" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="PCKO" direction="out"/>
<pin name="PCKI" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!IO16" direction="in"/>
<pin name="A" direction="in"/>
<pin name="!INDX" direction="in"/>
<pin name="FLGA" direction="out"/>
<pin name="FLGB" direction="out"/>
<pin name="CKO" direction="out"/>
<pin name="B" direction="in"/>
</symbol>
<symbol name="LS7766SO">
<pin name="DB0" direction="hiz"/>
<pin name="DB1" direction="hiz"/>
<pin name="DB2" direction="hiz"/>
<pin name="DB3" direction="hiz"/>
<pin name="DB4" direction="hiz"/>
<pin name="DB5" direction="hiz"/>
<pin name="DB6" direction="hiz"/>
<pin name="DB7" direction="hiz"/>
<pin name="RS0" direction="in"/>
<pin name="RS1" direction="in"/>
<pin name="RS2" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="PCKO" direction="out"/>
<pin name="PCKI" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="A" direction="in"/>
<pin name="!INDX" direction="in"/>
<pin name="FLGA" direction="out"/>
<pin name="FLGB" direction="out"/>
<pin name="CKO" direction="out"/>
<pin name="B" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LS7766DH" prefix="IC">
<description>&lt;b&gt;32-BIT SINGLE- AXIS/DUAL-AXIS QUADRATURE COUNTER&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Data_Sheets/LS7766.pdf</description>
<gates>
<gate name="G$1" symbol="LS7766DH"/>
</gates>
<devices>
<device name="-TS" package="TSSOP48">
<connects>
<connect gate="G$1" pin="!CS" pad="43"/>
<connect gate="G$1" pin="!IO16" pad="34"/>
<connect gate="G$1" pin="!RD" pad="45"/>
<connect gate="G$1" pin="!WR" pad="44"/>
<connect gate="G$1" pin="!X0!_X1" pad="33"/>
<connect gate="G$1" pin="!X0INDX" pad="28"/>
<connect gate="G$1" pin="!X1INDX" pad="39"/>
<connect gate="G$1" pin="DB0" pad="5"/>
<connect gate="G$1" pin="DB1" pad="6"/>
<connect gate="G$1" pin="DB10" pad="15"/>
<connect gate="G$1" pin="DB11" pad="16"/>
<connect gate="G$1" pin="DB12" pad="17"/>
<connect gate="G$1" pin="DB13" pad="18"/>
<connect gate="G$1" pin="DB14" pad="19"/>
<connect gate="G$1" pin="DB15" pad="20"/>
<connect gate="G$1" pin="DB2" pad="7"/>
<connect gate="G$1" pin="DB3" pad="8"/>
<connect gate="G$1" pin="DB4" pad="9"/>
<connect gate="G$1" pin="DB5" pad="10"/>
<connect gate="G$1" pin="DB6" pad="11"/>
<connect gate="G$1" pin="DB7" pad="12"/>
<connect gate="G$1" pin="DB8" pad="13"/>
<connect gate="G$1" pin="DB9" pad="14"/>
<connect gate="G$1" pin="PCKI" pad="46"/>
<connect gate="G$1" pin="PCKO" pad="47"/>
<connect gate="G$1" pin="RS0" pad="3"/>
<connect gate="G$1" pin="RS1" pad="2"/>
<connect gate="G$1" pin="RS2" pad="1"/>
<connect gate="G$1" pin="VDD" pad="48"/>
<connect gate="G$1" pin="VSS@1" pad="24"/>
<connect gate="G$1" pin="VSS@2" pad="35"/>
<connect gate="G$1" pin="X0A" pad="27"/>
<connect gate="G$1" pin="X0B" pad="26"/>
<connect gate="G$1" pin="X0CKO" pad="32"/>
<connect gate="G$1" pin="X0FLGA" pad="30"/>
<connect gate="G$1" pin="X0FLGB" pad="31"/>
<connect gate="G$1" pin="X1A" pad="40"/>
<connect gate="G$1" pin="X1B" pad="41"/>
<connect gate="G$1" pin="X1CKO" pad="36"/>
<connect gate="G$1" pin="X1FLGA" pad="38"/>
<connect gate="G$1" pin="X1FLGB" pad="37"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LS7766DO" prefix="IC">
<description>&lt;b&gt;32-BIT SINGLE- AXIS/DUAL-AXIS QUADRATURE COUNTER&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Data_Sheets/LS7766.pdf</description>
<gates>
<gate name="G$1" symbol="LS7766DO"/>
</gates>
<devices>
<device name="-S" package="SOIC28L">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="!RD" pad="5"/>
<connect gate="G$1" pin="!WR" pad="4"/>
<connect gate="G$1" pin="!X0!_X1" pad="25"/>
<connect gate="G$1" pin="!X0INDX" pad="22"/>
<connect gate="G$1" pin="!X1INDX" pad="28"/>
<connect gate="G$1" pin="DB0" pad="11"/>
<connect gate="G$1" pin="DB1" pad="12"/>
<connect gate="G$1" pin="DB2" pad="13"/>
<connect gate="G$1" pin="DB3" pad="14"/>
<connect gate="G$1" pin="DB4" pad="15"/>
<connect gate="G$1" pin="DB5" pad="16"/>
<connect gate="G$1" pin="DB6" pad="17"/>
<connect gate="G$1" pin="DB7" pad="18"/>
<connect gate="G$1" pin="PCKI" pad="6"/>
<connect gate="G$1" pin="RS0" pad="10"/>
<connect gate="G$1" pin="RS1" pad="9"/>
<connect gate="G$1" pin="RS2" pad="8"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="X0A" pad="21"/>
<connect gate="G$1" pin="X0B" pad="20"/>
<connect gate="G$1" pin="X0FLGA" pad="23"/>
<connect gate="G$1" pin="X0FLGB" pad="24"/>
<connect gate="G$1" pin="X1A" pad="1"/>
<connect gate="G$1" pin="X1B" pad="2"/>
<connect gate="G$1" pin="X1FLGA" pad="27"/>
<connect gate="G$1" pin="X1FLGB" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TS" package="TSSOP28">
<connects>
<connect gate="G$1" pin="!CS" pad="3"/>
<connect gate="G$1" pin="!RD" pad="5"/>
<connect gate="G$1" pin="!WR" pad="4"/>
<connect gate="G$1" pin="!X0!_X1" pad="25"/>
<connect gate="G$1" pin="!X0INDX" pad="22"/>
<connect gate="G$1" pin="!X1INDX" pad="28"/>
<connect gate="G$1" pin="DB0" pad="11"/>
<connect gate="G$1" pin="DB1" pad="12"/>
<connect gate="G$1" pin="DB2" pad="13"/>
<connect gate="G$1" pin="DB3" pad="14"/>
<connect gate="G$1" pin="DB4" pad="15"/>
<connect gate="G$1" pin="DB5" pad="16"/>
<connect gate="G$1" pin="DB6" pad="17"/>
<connect gate="G$1" pin="DB7" pad="18"/>
<connect gate="G$1" pin="PCKI" pad="6"/>
<connect gate="G$1" pin="RS0" pad="10"/>
<connect gate="G$1" pin="RS1" pad="9"/>
<connect gate="G$1" pin="RS2" pad="8"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VSS@1" pad="19"/>
<connect gate="G$1" pin="X0A" pad="21"/>
<connect gate="G$1" pin="X0B" pad="20"/>
<connect gate="G$1" pin="X0FLGA" pad="23"/>
<connect gate="G$1" pin="X0FLGB" pad="24"/>
<connect gate="G$1" pin="X1A" pad="1"/>
<connect gate="G$1" pin="X1B" pad="2"/>
<connect gate="G$1" pin="X1FLGA" pad="27"/>
<connect gate="G$1" pin="X1FLGB" pad="26"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LS7766SH" prefix="IC">
<description>&lt;b&gt;32-BIT SINGLE- AXIS/DUAL-AXIS QUADRATURE COUNTER&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Data_Sheets/LS7766.pdf</description>
<gates>
<gate name="G$1" symbol="LS7766SH"/>
</gates>
<devices>
<device name="-TS" package="TSSOP38">
<connects>
<connect gate="G$1" pin="!CS" pad="32"/>
<connect gate="G$1" pin="!INDX" pad="23"/>
<connect gate="G$1" pin="!IO16" pad="28"/>
<connect gate="G$1" pin="!RD" pad="35"/>
<connect gate="G$1" pin="!WR" pad="33"/>
<connect gate="G$1" pin="A" pad="22"/>
<connect gate="G$1" pin="B" pad="21"/>
<connect gate="G$1" pin="CKO" pad="26"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB10" pad="14"/>
<connect gate="G$1" pin="DB11" pad="15"/>
<connect gate="G$1" pin="DB12" pad="16"/>
<connect gate="G$1" pin="DB13" pad="17"/>
<connect gate="G$1" pin="DB14" pad="18"/>
<connect gate="G$1" pin="DB15" pad="19"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="DB8" pad="12"/>
<connect gate="G$1" pin="DB9" pad="13"/>
<connect gate="G$1" pin="FLGA" pad="24"/>
<connect gate="G$1" pin="FLGB" pad="25"/>
<connect gate="G$1" pin="PCKI" pad="36"/>
<connect gate="G$1" pin="PCKO" pad="37"/>
<connect gate="G$1" pin="RS0" pad="3"/>
<connect gate="G$1" pin="RS1" pad="2"/>
<connect gate="G$1" pin="RS2" pad="1"/>
<connect gate="G$1" pin="VDD" pad="38"/>
<connect gate="G$1" pin="VSS@1" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LS7766SO" prefix="IC">
<description>&lt;b&gt;32-BIT SINGLE- AXIS/DUAL-AXIS QUADRATURE COUNTER&lt;/b&gt;&lt;p&gt;
Source: http://www.lsicsi.com/pdfs/Data_Sheets/LS7766.pdf</description>
<gates>
<gate name="G$1" symbol="LS7766SO"/>
</gates>
<devices>
<device name="-S" package="SOIC24L">
<connects>
<connect gate="G$1" pin="!CS" pad="19"/>
<connect gate="G$1" pin="!INDX" pad="15"/>
<connect gate="G$1" pin="!RD" pad="21"/>
<connect gate="G$1" pin="!WR" pad="20"/>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="B" pad="13"/>
<connect gate="G$1" pin="CKO" pad="18"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="FLGA" pad="16"/>
<connect gate="G$1" pin="FLGB" pad="17"/>
<connect gate="G$1" pin="PCKI" pad="22"/>
<connect gate="G$1" pin="PCKO" pad="23"/>
<connect gate="G$1" pin="RS0" pad="3"/>
<connect gate="G$1" pin="RS1" pad="2"/>
<connect gate="G$1" pin="RS2" pad="1"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TS" package="TSSOP24">
<connects>
<connect gate="G$1" pin="!CS" pad="19"/>
<connect gate="G$1" pin="!INDX" pad="15"/>
<connect gate="G$1" pin="!RD" pad="21"/>
<connect gate="G$1" pin="!WR" pad="20"/>
<connect gate="G$1" pin="A" pad="14"/>
<connect gate="G$1" pin="B" pad="13"/>
<connect gate="G$1" pin="CKO" pad="18"/>
<connect gate="G$1" pin="DB0" pad="4"/>
<connect gate="G$1" pin="DB1" pad="5"/>
<connect gate="G$1" pin="DB2" pad="6"/>
<connect gate="G$1" pin="DB3" pad="7"/>
<connect gate="G$1" pin="DB4" pad="8"/>
<connect gate="G$1" pin="DB5" pad="9"/>
<connect gate="G$1" pin="DB6" pad="10"/>
<connect gate="G$1" pin="DB7" pad="11"/>
<connect gate="G$1" pin="FLGA" pad="16"/>
<connect gate="G$1" pin="FLGB" pad="17"/>
<connect gate="G$1" pin="PCKI" pad="22"/>
<connect gate="G$1" pin="PCKO" pad="23"/>
<connect gate="G$1" pin="RS0" pad="3"/>
<connect gate="G$1" pin="RS1" pad="2"/>
<connect gate="G$1" pin="RS2" pad="1"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
