<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Cyrod Technologies Inc.&lt;/b&gt;&lt;p&gt;
www.cyrod.com</description>
<packages>
<package name="TQFP64L-10X10X2.0MM">
<description>&lt;b&gt;TQFP 64L-10X10X2.0 MM&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;
Source: www.cyrod.com .. CRD89C51RD1T-V10.pdf</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="SQFP-S-10X10-44">
<description>&lt;b&gt;QFP44&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 600mil</description>
</package>
</packages>
<symbols>
<symbol name="CRD89C51RD1T">
<pin name="P5_2"/>
<pin name="P5_3"/>
<pin name="P5_4"/>
<pin name="P5_5"/>
<pin name="P5_6"/>
<pin name="P5_7"/>
<pin name="VDD_IO" direction="pwr"/>
<pin name="VSS_IO" direction="pwr"/>
<pin name="P4_0/PWM2"/>
<pin name="P4_1/PWM3"/>
<pin name="P42"/>
<pin name="P43"/>
<pin name="P4_4/ADC0"/>
<pin name="P4_5/ADC1"/>
<pin name="P4_6/ADC2"/>
<pin name="P4_7/ADC3"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="P1_7/IIC_SDA"/>
<pin name="P1_6/IIC_SCL"/>
<pin name="P1_5/PWM1/CC1"/>
<pin name="P1_4/PWM0/CC0"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVDD_3V" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="P1_3/TXD1/CC3/SPI_MOSI"/>
<pin name="P1_2/RXD1/CC2/SPI_MISO"/>
<pin name="P1_1/T2EX/SPI_CLK"/>
<pin name="P1_0/T2/SPI_SS"/>
<pin name="P2_7/A15"/>
<pin name="P2_6/A14"/>
<pin name="P2_5/A13"/>
<pin name="P2_4/A12"/>
<pin name="P2_3/A11"/>
<pin name="P2_2/A10"/>
<pin name="P2_1/A9"/>
<pin name="P2_0/A8"/>
<pin name="P3_7/RD"/>
<pin name="P3_6/WR"/>
<pin name="P3_5/T1"/>
<pin name="P3_4/T0"/>
<pin name="P3_3/INT1"/>
<pin name="P3_2/INT0"/>
<pin name="P3_1/TXD0"/>
<pin name="P3_0/RXD0"/>
<pin name="P0_7/AD7"/>
<pin name="P0_6/AD6"/>
<pin name="P0_5/AD5"/>
<pin name="P0_4/AD4"/>
<pin name="P0_3/AD3"/>
<pin name="P0_2/AD2"/>
<pin name="P0_1/AD1"/>
<pin name="P0_0/AD0"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD_3V" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="ICE_ICP_BUSY" direction="out"/>
<pin name="ICE_ICP_DATA"/>
<pin name="ICE_ICP_CLOCK"/>
<pin name="ALE" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="P5_0"/>
<pin name="P5_1"/>
</symbol>
<symbol name="CRD89C51RD-PLCC44">
<pin name="P4_2"/>
<pin name="P1_0/T2"/>
<pin name="P1_1/T2EX"/>
<pin name="P1_2"/>
<pin name="P1_3/SPWM0"/>
<pin name="P1_4/SPWM1"/>
<pin name="P1_5/SPWM2"/>
<pin name="P1_6/SPWM3"/>
<pin name="P1_7/SPWM4"/>
<pin name="RES" direction="in"/>
<pin name="P3_0/RXD"/>
<pin name="P4_3"/>
<pin name="P3_1/TXD"/>
<pin name="P3_2/!INT0"/>
<pin name="P3_3/!INT1"/>
<pin name="P3_4/T0"/>
<pin name="P3_5/T1"/>
<pin name="P3_6/!WR"/>
<pin name="P3_7/!RD"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="P4_0"/>
<pin name="P2_0/A8"/>
<pin name="P2_1/A9"/>
<pin name="P2_2/A10"/>
<pin name="P2_3/A11"/>
<pin name="P2_4/A12"/>
<pin name="P2_5/A13"/>
<pin name="P2_6/A14"/>
<pin name="P2_7/A15"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="P4_1"/>
<pin name="!EA" direction="in"/>
<pin name="P0_7/AD7"/>
<pin name="P0_6/AD6"/>
<pin name="P0_5/AD5"/>
<pin name="P0_4/AD4"/>
<pin name="P0_3/AD3"/>
<pin name="P0_2/AD2"/>
<pin name="P0_1/AD1"/>
<pin name="P0_0/AD0"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="CRD89C51RD-QFP44">
<pin name="P1_5/SPWM2"/>
<pin name="P1_6/SPWM3"/>
<pin name="P1_7/SPWM4"/>
<pin name="RES" direction="in"/>
<pin name="P3_0/RXD"/>
<pin name="P4_3"/>
<pin name="P3_1/TXD"/>
<pin name="P3_2/!INT0"/>
<pin name="P3_3/!INT1"/>
<pin name="P3_4/T0"/>
<pin name="P3_5/T1"/>
<pin name="P3_6/!WR"/>
<pin name="P3_7/!RD"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="P4_0"/>
<pin name="P2_0/A8"/>
<pin name="P2_1/A9"/>
<pin name="P2_2/A10"/>
<pin name="P2_3/A11"/>
<pin name="P2_4/A12"/>
<pin name="P2_5/A13"/>
<pin name="P2_6/A14"/>
<pin name="P2_7/A15"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="P4_1"/>
<pin name="!EA" direction="in"/>
<pin name="P0_7/AD7"/>
<pin name="P0_6/AD6"/>
<pin name="P0_5/AD5"/>
<pin name="P0_4/AD4"/>
<pin name="P0_3/AD3"/>
<pin name="P0_2/AD2"/>
<pin name="P0_1/AD1"/>
<pin name="P0_0/AD0"/>
<pin name="VDD" direction="pwr"/>
<pin name="P4_2"/>
<pin name="P1_0/T2"/>
<pin name="P1_1/T2EX"/>
<pin name="P1_2"/>
<pin name="P1_3/SPWM0"/>
<pin name="P1_4/SPWM1"/>
</symbol>
<symbol name="CRD89C51RD-DIL40">
<pin name="P1_0/T2"/>
<pin name="P1_1/T2EX"/>
<pin name="P1_2"/>
<pin name="P1_3/SPWM0"/>
<pin name="P1_4/SPWM1"/>
<pin name="P1_5/SPWM2"/>
<pin name="P1_6/SPWM3"/>
<pin name="P1_7/SPWM4"/>
<pin name="RES" direction="in"/>
<pin name="P3_0/RXD"/>
<pin name="P3_1/TXD"/>
<pin name="P3_2/!INT0"/>
<pin name="P3_3/!INT1"/>
<pin name="P3_4/T0"/>
<pin name="P3_5/T1"/>
<pin name="P3_6/!WR"/>
<pin name="P3_7/!RD"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="P2_0/A8"/>
<pin name="P2_1/A9"/>
<pin name="P2_2/A10"/>
<pin name="P2_3/A11"/>
<pin name="P2_4/A12"/>
<pin name="P2_5/A13"/>
<pin name="P2_6/A14"/>
<pin name="P2_7/A15"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="P0_7/AD7"/>
<pin name="P0_6/AD6"/>
<pin name="P0_5/AD5"/>
<pin name="P0_4/AD4"/>
<pin name="P0_3/AD3"/>
<pin name="P0_2/AD2"/>
<pin name="P0_1/AD1"/>
<pin name="P0_0/AD0"/>
<pin name="VDD" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CRD89C51RD1T" prefix="IC">
<description>&lt;b&gt;8 bit, fast, microcontroller with 64KB program/ISP Flash and 2KB RAM&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;
Source: www.cyrod.com .. CRD89C51RD1T-V10.pdf</description>
<gates>
<gate name="G$1" symbol="CRD89C51RD1T"/>
</gates>
<devices>
<device name="" package="TQFP64L-10X10X2.0MM">
<connects>
<connect gate="G$1" pin="ALE" pad="61"/>
<connect gate="G$1" pin="AVDD" pad="24"/>
<connect gate="G$1" pin="AVDD_3V" pad="25"/>
<connect gate="G$1" pin="AVSS" pad="26"/>
<connect gate="G$1" pin="ICE_ICP_BUSY" pad="58"/>
<connect gate="G$1" pin="ICE_ICP_CLOCK" pad="60"/>
<connect gate="G$1" pin="ICE_ICP_DATA" pad="59"/>
<connect gate="G$1" pin="NC" pad="19"/>
<connect gate="G$1" pin="P0_0/AD0" pad="54"/>
<connect gate="G$1" pin="P0_1/AD1" pad="53"/>
<connect gate="G$1" pin="P0_2/AD2" pad="52"/>
<connect gate="G$1" pin="P0_3/AD3" pad="51"/>
<connect gate="G$1" pin="P0_4/AD4" pad="50"/>
<connect gate="G$1" pin="P0_5/AD5" pad="49"/>
<connect gate="G$1" pin="P0_6/AD6" pad="48"/>
<connect gate="G$1" pin="P0_7/AD7" pad="47"/>
<connect gate="G$1" pin="P1_0/T2/SPI_SS" pad="30"/>
<connect gate="G$1" pin="P1_1/T2EX/SPI_CLK" pad="29"/>
<connect gate="G$1" pin="P1_2/RXD1/CC2/SPI_MISO" pad="28"/>
<connect gate="G$1" pin="P1_3/TXD1/CC3/SPI_MOSI" pad="27"/>
<connect gate="G$1" pin="P1_4/PWM0/CC0" pad="23"/>
<connect gate="G$1" pin="P1_5/PWM1/CC1" pad="22"/>
<connect gate="G$1" pin="P1_6/IIC_SCL" pad="21"/>
<connect gate="G$1" pin="P1_7/IIC_SDA" pad="20"/>
<connect gate="G$1" pin="P2_0/A8" pad="38"/>
<connect gate="G$1" pin="P2_1/A9" pad="37"/>
<connect gate="G$1" pin="P2_2/A10" pad="36"/>
<connect gate="G$1" pin="P2_3/A11" pad="35"/>
<connect gate="G$1" pin="P2_4/A12" pad="34"/>
<connect gate="G$1" pin="P2_5/A13" pad="33"/>
<connect gate="G$1" pin="P2_6/A14" pad="32"/>
<connect gate="G$1" pin="P2_7/A15" pad="31"/>
<connect gate="G$1" pin="P3_0/RXD0" pad="46"/>
<connect gate="G$1" pin="P3_1/TXD0" pad="45"/>
<connect gate="G$1" pin="P3_2/INT0" pad="44"/>
<connect gate="G$1" pin="P3_3/INT1" pad="43"/>
<connect gate="G$1" pin="P3_4/T0" pad="42"/>
<connect gate="G$1" pin="P3_5/T1" pad="41"/>
<connect gate="G$1" pin="P3_6/WR" pad="40"/>
<connect gate="G$1" pin="P3_7/RD" pad="39"/>
<connect gate="G$1" pin="P42" pad="11"/>
<connect gate="G$1" pin="P43" pad="12"/>
<connect gate="G$1" pin="P4_0/PWM2" pad="9"/>
<connect gate="G$1" pin="P4_1/PWM3" pad="10"/>
<connect gate="G$1" pin="P4_4/ADC0" pad="13"/>
<connect gate="G$1" pin="P4_5/ADC1" pad="14"/>
<connect gate="G$1" pin="P4_6/ADC2" pad="15"/>
<connect gate="G$1" pin="P4_7/ADC3" pad="16"/>
<connect gate="G$1" pin="P5_0" pad="63"/>
<connect gate="G$1" pin="P5_1" pad="64"/>
<connect gate="G$1" pin="P5_2" pad="1"/>
<connect gate="G$1" pin="P5_3" pad="2"/>
<connect gate="G$1" pin="P5_4" pad="3"/>
<connect gate="G$1" pin="P5_5" pad="4"/>
<connect gate="G$1" pin="P5_6" pad="5"/>
<connect gate="G$1" pin="P5_7" pad="6"/>
<connect gate="G$1" pin="RESET" pad="62"/>
<connect gate="G$1" pin="VDD" pad="57"/>
<connect gate="G$1" pin="VDD_3V" pad="56"/>
<connect gate="G$1" pin="VDD_IO" pad="7"/>
<connect gate="G$1" pin="VSS" pad="55"/>
<connect gate="G$1" pin="VSS_IO" pad="8"/>
<connect gate="G$1" pin="XTAL1" pad="17"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRD89C51RD" prefix="IC">
<description>&lt;b&gt;CRD89C51RD series 8 - bit single chip micro controller unit (MCU) with 64KB flash &amp; 1K byte RAM embedded.&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source: CRD89C51RD_v001.pdf</description>
<gates>
<gate name="G$1" symbol="CRD89C51RD-PLCC44"/>
</gates>
<devices>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="!EA" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="32"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="P0_0/AD0" pad="43"/>
<connect gate="G$1" pin="P0_1/AD1" pad="42"/>
<connect gate="G$1" pin="P0_2/AD2" pad="41"/>
<connect gate="G$1" pin="P0_3/AD3" pad="40"/>
<connect gate="G$1" pin="P0_4/AD4" pad="39"/>
<connect gate="G$1" pin="P0_5/AD5" pad="38"/>
<connect gate="G$1" pin="P0_6/AD6" pad="37"/>
<connect gate="G$1" pin="P0_7/AD7" pad="36"/>
<connect gate="G$1" pin="P1_0/T2" pad="2"/>
<connect gate="G$1" pin="P1_1/T2EX" pad="3"/>
<connect gate="G$1" pin="P1_2" pad="4"/>
<connect gate="G$1" pin="P1_3/SPWM0" pad="5"/>
<connect gate="G$1" pin="P1_4/SPWM1" pad="6"/>
<connect gate="G$1" pin="P1_5/SPWM2" pad="7"/>
<connect gate="G$1" pin="P1_6/SPWM3" pad="8"/>
<connect gate="G$1" pin="P1_7/SPWM4" pad="9"/>
<connect gate="G$1" pin="P2_0/A8" pad="24"/>
<connect gate="G$1" pin="P2_1/A9" pad="25"/>
<connect gate="G$1" pin="P2_2/A10" pad="26"/>
<connect gate="G$1" pin="P2_3/A11" pad="27"/>
<connect gate="G$1" pin="P2_4/A12" pad="28"/>
<connect gate="G$1" pin="P2_5/A13" pad="29"/>
<connect gate="G$1" pin="P2_6/A14" pad="30"/>
<connect gate="G$1" pin="P2_7/A15" pad="31"/>
<connect gate="G$1" pin="P3_0/RXD" pad="11"/>
<connect gate="G$1" pin="P3_1/TXD" pad="13"/>
<connect gate="G$1" pin="P3_2/!INT0" pad="14"/>
<connect gate="G$1" pin="P3_3/!INT1" pad="15"/>
<connect gate="G$1" pin="P3_4/T0" pad="16"/>
<connect gate="G$1" pin="P3_5/T1" pad="17"/>
<connect gate="G$1" pin="P3_6/!WR" pad="18"/>
<connect gate="G$1" pin="P3_7/!RD" pad="19"/>
<connect gate="G$1" pin="P4_0" pad="23"/>
<connect gate="G$1" pin="P4_1" pad="34"/>
<connect gate="G$1" pin="P4_2" pad="1"/>
<connect gate="G$1" pin="P4_3" pad="12"/>
<connect gate="G$1" pin="RES" pad="10"/>
<connect gate="G$1" pin="VDD" pad="44"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRD89C51RD-QFP44" prefix="IC">
<description>&lt;b&gt;CRD89C51RD series 8 - bit single chip micro controller unit (MCU) with 64KB flash &amp; 1K byte RAM embedded.&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source: CRD89C51RD_v001.pdf</description>
<gates>
<gate name="G$1" symbol="CRD89C51RD-QFP44"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-44">
<connects>
<connect gate="G$1" pin="!EA" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="P0_0/AD0" pad="37"/>
<connect gate="G$1" pin="P0_1/AD1" pad="36"/>
<connect gate="G$1" pin="P0_2/AD2" pad="35"/>
<connect gate="G$1" pin="P0_3/AD3" pad="34"/>
<connect gate="G$1" pin="P0_4/AD4" pad="33"/>
<connect gate="G$1" pin="P0_5/AD5" pad="32"/>
<connect gate="G$1" pin="P0_6/AD6" pad="31"/>
<connect gate="G$1" pin="P0_7/AD7" pad="30"/>
<connect gate="G$1" pin="P1_0/T2" pad="40"/>
<connect gate="G$1" pin="P1_1/T2EX" pad="41"/>
<connect gate="G$1" pin="P1_2" pad="42"/>
<connect gate="G$1" pin="P1_3/SPWM0" pad="43"/>
<connect gate="G$1" pin="P1_4/SPWM1" pad="44"/>
<connect gate="G$1" pin="P1_5/SPWM2" pad="1"/>
<connect gate="G$1" pin="P1_6/SPWM3" pad="2"/>
<connect gate="G$1" pin="P1_7/SPWM4" pad="3"/>
<connect gate="G$1" pin="P2_0/A8" pad="18"/>
<connect gate="G$1" pin="P2_1/A9" pad="19"/>
<connect gate="G$1" pin="P2_2/A10" pad="20"/>
<connect gate="G$1" pin="P2_3/A11" pad="21"/>
<connect gate="G$1" pin="P2_4/A12" pad="22"/>
<connect gate="G$1" pin="P2_5/A13" pad="23"/>
<connect gate="G$1" pin="P2_6/A14" pad="24"/>
<connect gate="G$1" pin="P2_7/A15" pad="25"/>
<connect gate="G$1" pin="P3_0/RXD" pad="5"/>
<connect gate="G$1" pin="P3_1/TXD" pad="7"/>
<connect gate="G$1" pin="P3_2/!INT0" pad="8"/>
<connect gate="G$1" pin="P3_3/!INT1" pad="9"/>
<connect gate="G$1" pin="P3_4/T0" pad="10"/>
<connect gate="G$1" pin="P3_5/T1" pad="11"/>
<connect gate="G$1" pin="P3_6/!WR" pad="12"/>
<connect gate="G$1" pin="P3_7/!RD" pad="13"/>
<connect gate="G$1" pin="P4_0" pad="17"/>
<connect gate="G$1" pin="P4_1" pad="28"/>
<connect gate="G$1" pin="P4_2" pad="39"/>
<connect gate="G$1" pin="P4_3" pad="6"/>
<connect gate="G$1" pin="RES" pad="4"/>
<connect gate="G$1" pin="VDD" pad="38"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="XTAL1" pad="15"/>
<connect gate="G$1" pin="XTAL2" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRD89C51RD-DIL40" prefix="IC">
<description>&lt;b&gt;CRD89C51RD series 8 - bit single chip micro controller unit (MCU) with 64KB flash &amp; 1K byte RAM embedded.&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source: CRD89C51RD_v001.pdf</description>
<gates>
<gate name="G$1" symbol="CRD89C51RD-DIL40"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!EA" pad="31"/>
<connect gate="G$1" pin="!PSEN" pad="29"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="P0_0/AD0" pad="39"/>
<connect gate="G$1" pin="P0_1/AD1" pad="38"/>
<connect gate="G$1" pin="P0_2/AD2" pad="37"/>
<connect gate="G$1" pin="P0_3/AD3" pad="36"/>
<connect gate="G$1" pin="P0_4/AD4" pad="35"/>
<connect gate="G$1" pin="P0_5/AD5" pad="34"/>
<connect gate="G$1" pin="P0_6/AD6" pad="33"/>
<connect gate="G$1" pin="P0_7/AD7" pad="32"/>
<connect gate="G$1" pin="P1_0/T2" pad="1"/>
<connect gate="G$1" pin="P1_1/T2EX" pad="2"/>
<connect gate="G$1" pin="P1_2" pad="3"/>
<connect gate="G$1" pin="P1_3/SPWM0" pad="4"/>
<connect gate="G$1" pin="P1_4/SPWM1" pad="5"/>
<connect gate="G$1" pin="P1_5/SPWM2" pad="6"/>
<connect gate="G$1" pin="P1_6/SPWM3" pad="7"/>
<connect gate="G$1" pin="P1_7/SPWM4" pad="8"/>
<connect gate="G$1" pin="P2_0/A8" pad="21"/>
<connect gate="G$1" pin="P2_1/A9" pad="22"/>
<connect gate="G$1" pin="P2_2/A10" pad="23"/>
<connect gate="G$1" pin="P2_3/A11" pad="24"/>
<connect gate="G$1" pin="P2_4/A12" pad="25"/>
<connect gate="G$1" pin="P2_5/A13" pad="26"/>
<connect gate="G$1" pin="P2_6/A14" pad="27"/>
<connect gate="G$1" pin="P2_7/A15" pad="28"/>
<connect gate="G$1" pin="P3_0/RXD" pad="10"/>
<connect gate="G$1" pin="P3_1/TXD" pad="11"/>
<connect gate="G$1" pin="P3_2/!INT0" pad="12"/>
<connect gate="G$1" pin="P3_3/!INT1" pad="13"/>
<connect gate="G$1" pin="P3_4/T0" pad="14"/>
<connect gate="G$1" pin="P3_5/T1" pad="15"/>
<connect gate="G$1" pin="P3_6/!WR" pad="16"/>
<connect gate="G$1" pin="P3_7/!RD" pad="17"/>
<connect gate="G$1" pin="RES" pad="9"/>
<connect gate="G$1" pin="VDD" pad="40"/>
<connect gate="G$1" pin="VSS" pad="20"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
