<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.2">
<drawing>
<library>
<description>&lt;b&gt;Philips Microcontroller Devices&lt;/b&gt;&lt;p&gt;
http://www-eu2.semiconductors.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="QFP12-80">
<description>&lt;b&gt;Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PLCC68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="QFP100R">
<description>&lt;b&gt;Quad Flat Pack Package&lt;/b&gt; 100 Pin Rectangle</description>
</package>
<package name="QFP80R">
<description>&lt;b&gt;Quad Flat Pack Package&lt;/b&gt; 80 Pin Rectangle</description>
</package>
<package name="LOGO10">
<description>&lt;b&gt;LOGO&lt;/b&gt; 10 mm</description>
</package>
<package name="LOGO5">
<description>&lt;b&gt;LOGO&lt;/b&gt; 5 mm</description>
</package>
<package name="SOT353">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="I2C">
<description>&lt;b&gt;I2C LOGO&lt;/b&gt;</description>
</package>
<package name="SO24">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; 7.6 x 15.74 mm</description>
</package>
<package name="DIL24-6">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO16W">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; 7.6 x 10.6 mm</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO28">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; 7.6 x 18.3 mm</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SSOP16">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SO8-7_5">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="SO20W">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; 7.6 x 13.2 mm</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; 4 x 10 mm</description>
</package>
<package name="SSOP24">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;&lt;p&gt;
SOT340-1 / JEDEC MO-150AG</description>
</package>
<package name="SCQFP44">
<description>&lt;b&gt;CERAMIC QUAD FLAT PACK&lt;/b&gt;</description>
</package>
<package name="QFP44_SOT307-2">
<description>&lt;b&gt;Plastic Quad Flat Package SOT307-2&lt;/b&gt;&lt;p&gt;
44 leads (lead length 1.3 mm); body 10 x 10 x 1.75 mm SOT307-2&lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="PLCC44S">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="LCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="QFP44_SOT205-1">
<description>&lt;b&gt;Plastic Quad Flat Package SOT205-1&lt;/b&gt; 44 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP52_SOT379-1">
<description>&lt;b&gt;Plastic Quad Flat Package SOT379-1&lt;/b&gt; 52 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP64_SOT319">
<description>&lt;b&gt;Plastic Quad Flat Package SOT319-1/-2/-5&lt;/b&gt; 64 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP64_SOT393">
<description>&lt;b&gt;Plastic Quad Flat Package SOT393-1/-2&lt;/b&gt; 64 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP80_SOT310-1">
<description>&lt;b&gt;Plastic Quad Flat Package SOT310-1&lt;/b&gt; 80 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP80_SOT318">
<description>&lt;b&gt;Plastic Quad Flat Package SOT318-1/-2&lt;/b&gt; 80 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP80_SOT496-1">
<description>&lt;b&gt;Plastic Quad Flat Package SOT496&lt;/b&gt; 80 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP100_SOT317-SOT382-2">
<description>&lt;b&gt;Plastic Quad Flat Package SOT317-1/-2/-3 SOT382-2&lt;/b&gt; 100 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP100_SOT382-1">
<description>&lt;b&gt;Plastic Quad Flat Package SOT382-1&lt;/b&gt; 100 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP120_SOT349-2">
<description>&lt;b&gt;Plastic Quad Flat Package SOT349-2&lt;/b&gt; 120 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="QFP128_SOT320-2">
<description>&lt;b&gt;Plastic Quad Flat Package SOT320-2&lt;/b&gt; 120 leads &lt;p&gt;
source: http://www.semiconductors.philips.com/&lt;p&gt;
LQFP-MSQFP-QFP-SQFP-TQFP-REFLOW.pdf</description>
</package>
<package name="PLCC-S68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt; Socked</description>
</package>
<package name="PQFP-44">
<description>&lt;b&gt;Plastic Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="DIP24SKI">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="QFP80">
<description>&lt;b&gt;Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="DIL28">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SOT136A">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="SO-28L">
<description>&lt;b&gt;Small Outline large&lt;/b&gt;</description>
</package>
<package name="LFBGA96">
<description>&lt;b&gt;LFBGA96&lt;/b&gt; SOT536-1&lt;p&gt;
plastic low profile fine-pitch ball grid array package&lt;br&gt;
96 balls; body 13.5 x 5.5 x 1.05 mm&lt;br&gt;
SOT536-1.pdf</description>
</package>
<package name="HBCC16">
<description>&lt;b&gt;HBCC16&lt;/b&gt; plastic thermal enhanced bottom chip carrier SOT639-2&lt;br&gt;
16 terminals; body 3 x 3 x 0.65 mm&lt;br&gt;
Source: http://www.semiconductors.philips.com/cgi-bin/pldb/package/sot639-2.html</description>
</package>
<package name="HVQFN24">
<description>&lt;b&gt;plastic thermal enhanced very thin quad flat package&lt;/b&gt; SOT616-1&lt;p&gt;
no leads; 24 terminals; body 4 x 4 x 0.85 mm&lt;br&gt;
Source: PCA9555_5.pdf</description>
</package>
<package name="TSSOP24">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 24&lt;/b&gt;&lt;p&gt;
Source: MAX3223-MAX3243.pdf</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;plastic shrink small outline package&lt;/b&gt; 20 leads; body width 4.4 mm SOT266-1&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/PCF8574_4.pdf</description>
</package>
<package name="HVQFN32">
<description>&lt;b&gt;HVQFN32 (SOT617-3)&lt;/b&gt; plastic thermal enhanced very thin quad flat package; no leads&lt;p&gt;
32 terminals; body 5 x 5 x 0.85 mm
Source: http://www.semiconductors.philips.com/acrobat_download/packages/SOT617-3.pdf</description>
</package>
<package name="HVQFN40">
<description>&lt;b&gt;HVQFN40&lt;/b&gt; plastic thermal enhanced very thin quad flat package SOT618-1&lt;p&gt;
no leads; 40 terminals; body 6 x 6 x 0.85 mm&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/packages/SOT618-1.pdf</description>
</package>
<package name="HLLGA48R">
<description>&lt;b&gt;HLLGA48R&lt;/b&gt; (SOT863-1) plastic thermal enhanced low profile land grid array package, body 8 x 7 x 1.4 mm&lt;p&gt;
Source: NXP Semiconductors  SOT863-1.pdf</description>
</package>
<package name="PLCC28S">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="HVQFN28">
<description>&lt;b&gt;HVQFN28: plastic thermal enhanced very thin quad flat package&lt;/b&gt; SOT788-1&lt;p&gt;
no leads; 28 terminals; body 6 x 6 x 0.85 mm&lt;br&gt;
Source: &lt;a href="http://www.nxp.com/documents/data_sheet/P89LPC933_934_935_936.pdf"&gt; Data sheet&lt;/a&gt;</description>
</package>
<package name="TSSOP56-6">
<description>&lt;b&gt;TSSOP56&lt;/b&gt; Plastic thin shrink small outline package; 56 leads; body width 6.1mm AKA SOT364-1&lt;p&gt;
Source: http://www.nxp.com/acrobat_download/datasheets/PCA9505_9506_3.pdf</description>
</package>
<package name="SO8">
<description>&lt;B&gt;SO8: plastic small outline package; 8 leads; body width 3.9 mm&lt;/B&gt;&lt;p&gt;
Source: http://www.nxp.com/documents/data_sheet/PCA82C250.pdf</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;TSSOP16: plastic thin shrink small outline package; 16 leads; body width 4.4 mm&lt;/b&gt; SOT403-1&lt;p&gt;
Source: PCA9534_3.pdf</description>
</package>
<package name="HVQFN16_4X4">
<description>&lt;b&gt;HVQFN16: plastic thermal enhanced very thin quad flat package; no leads; 16 terminals; body 4 x 4 x 0.85 mm&lt;/b&gt; SOT629-1&lt;p&gt;
Source: PCA9534_3.pdf</description>
</package>
<package name="HVQFN16_3X3">
<description>&lt;b&gt;HVQFN16: plastic thermal enhanced very thin quad flat package; no leads; 16 terminals; body 3 x 3 x 0.85 mm&lt;/b&gt; SOT758-1&lt;p&gt;
Source: PCA9534_3.pdf</description>
</package>
<package name="WLCSP16">
<description>&lt;b&gt;WLCSP16: wafer level chip-size package; 16 bumps; body 2.17 x 2.32 x 0.6 mm&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://ics.nxp.com/products/lpc1000/datasheet/lpc1102.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
<symbols>
<symbol name="P90CL301">
<pin name="HALT"/>
<pin name="RESET"/>
<pin name="RESETIN" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="SP0/INT0/"/>
<pin name="SP1/INT1/"/>
<pin name="SP2/INT2/"/>
<pin name="SP3/INT3/"/>
<pin name="SP4/INT4"/>
<pin name="SP5/INT5"/>
<pin name="SP6/INT6"/>
<pin name="SP7/NMIN"/>
<pin name="P8/PWM0"/>
<pin name="P9/PWM1"/>
<pin name="P10/SCL"/>
<pin name="P11/SDA"/>
<pin name="P12/ADC0"/>
<pin name="P13/ADC1"/>
<pin name="P14/ADC2"/>
<pin name="P15/ADC3"/>
<pin name="UDS/A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="PCS0/A19" direction="out"/>
<pin name="PCS1/A20" direction="out"/>
<pin name="PCS2/A21" direction="out"/>
<pin name="PCS3/A22" direction="out"/>
<pin name="CS6/A23" direction="out"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8/P0"/>
<pin name="D9/P1"/>
<pin name="D10/P2"/>
<pin name="D11/P3"/>
<pin name="D12/P4"/>
<pin name="D13/P5"/>
<pin name="D14/P6"/>
<pin name="D15/P7"/>
<pin name="AS" direction="out"/>
<pin name="TROM_R/W"/>
<pin name="CS5/WR" direction="out"/>
<pin name="DTACK" direction="out"/>
<pin name="BSIZE" direction="out"/>
<pin name="VREF" direction="pas"/>
<pin name="LDS/DS" direction="out"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="CS0/FC0"/>
<pin name="CS1/FC1"/>
<pin name="CS2/FC2"/>
<pin name="CS3/ALE" direction="out"/>
<pin name="CS4/RD" direction="out"/>
<pin name="CSBT/ONCE"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VSSA" direction="pwr"/>
</symbol>
<symbol name="80C552">
<pin name="AD0-P0.0"/>
<pin name="AD1-P0.1"/>
<pin name="AD2-P0.2"/>
<pin name="AD3-P0.3"/>
<pin name="AD4-P0.4"/>
<pin name="AD5-P0.5"/>
<pin name="AD6-P0.6"/>
<pin name="AD7-P0.7"/>
<pin name="CT0I-P1.0"/>
<pin name="CT1I-P1.1"/>
<pin name="CT2I-P1.2"/>
<pin name="CT3I-P1.3"/>
<pin name="T2-P1.4"/>
<pin name="RT2-P1.5"/>
<pin name="CSL-P1.6"/>
<pin name="SDA-P1.7"/>
<pin name="A08-P2.0"/>
<pin name="A09-P2.1"/>
<pin name="A10-P2.2"/>
<pin name="A11-P2.3"/>
<pin name="A12-P2.4"/>
<pin name="A13-P2.5"/>
<pin name="A14-P2.6"/>
<pin name="A15-P2.7"/>
<pin name="P3.0-RXD"/>
<pin name="P3.1-TXD"/>
<pin name="P3.2-INT0/"/>
<pin name="P3.3-INT1/"/>
<pin name="P3.4-T0"/>
<pin name="P3.5-T1"/>
<pin name="P3.6-WR/"/>
<pin name="P3.7-RD/"/>
<pin name="P4.0-CMSR0"/>
<pin name="P4.1-CMSR1"/>
<pin name="P4.2-CMSR2"/>
<pin name="P4.3-CMSR3"/>
<pin name="P4.4-CMSR4"/>
<pin name="P4.5-CMSR5"/>
<pin name="P4.6-CMT0"/>
<pin name="P4.7-CMT1"/>
<pin name="P5.0-ADC0"/>
<pin name="P5.1-ADC1"/>
<pin name="P5.2-ADC2"/>
<pin name="P5.3-ADC3"/>
<pin name="P5.4-ADC4"/>
<pin name="P5.5-ADC5"/>
<pin name="P5.6-ADC6"/>
<pin name="P5.7-ADC7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="EA/VPP" direction="in"/>
<pin name="ALE-PROG/" direction="out"/>
<pin name="PSEN/" direction="out"/>
<pin name="RST"/>
<pin name="EW/" direction="in"/>
<pin name="STADC" direction="in"/>
<pin name="AVREF-" direction="in"/>
<pin name="AVREF+" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="AVSS" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="PWM0/" direction="out"/>
<pin name="PWM1/" direction="out"/>
<pin name="NC3" direction="nc"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="VSS">
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="NU">
<pin name="IC-NU" direction="nc"/>
</symbol>
<symbol name="LOGO20">
</symbol>
<symbol name="LOGO10">
</symbol>
<symbol name="SAA1064">
<pin name="SCL" direction="in"/>
<pin name="SDA" direction="in"/>
<pin name="CEXT" direction="in"/>
<pin name="ADR" direction="in"/>
<pin name="MX1" direction="out"/>
<pin name="MX2" direction="out"/>
<pin name="P1" direction="out"/>
<pin name="P2" direction="out"/>
<pin name="P3" direction="out"/>
<pin name="P4" direction="out"/>
<pin name="P5" direction="out"/>
<pin name="P6" direction="out"/>
<pin name="P7" direction="out"/>
<pin name="P8" direction="out"/>
<pin name="P9" direction="out"/>
<pin name="P10" direction="out"/>
<pin name="P11" direction="out"/>
<pin name="P12" direction="out"/>
<pin name="P13" direction="out"/>
<pin name="P14" direction="out"/>
<pin name="P15" direction="out"/>
<pin name="P16" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
</symbol>
<symbol name="PCF8573">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="COMP" direction="out"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="EXTPF" direction="in"/>
<pin name="PFIN" direction="in"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="MIN" direction="out"/>
<pin name="SEC" direction="out"/>
<pin name="FSET" direction="out"/>
<pin name="TEST" direction="in"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PCF8591">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="EXT" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="AIN0" direction="in"/>
<pin name="AIN1" direction="in"/>
<pin name="AIN2" direction="in"/>
<pin name="AIN3" direction="in"/>
<pin name="AOUT" direction="out"/>
<pin name="VREF" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PCF8574">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
</symbol>
<symbol name="P82C150">
<pin name="TX1" direction="out"/>
<pin name="TX0" direction="out"/>
<pin name="REF" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="XMOD" direction="in"/>
<pin name="RX0" direction="in"/>
<pin name="RX1" direction="in"/>
<pin name="AVDD" direction="in"/>
<pin name="AVSS" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CLK/P0"/>
<pin name="P1"/>
<pin name="P2"/>
<pin name="P3"/>
<pin name="P4"/>
<pin name="P5"/>
<pin name="P6"/>
<pin name="P7"/>
<pin name="P8"/>
<pin name="P9"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
<pin name="P15"/>
<pin name="P16"/>
</symbol>
<symbol name="P82C250">
<pin name="TXD" direction="in"/>
<pin name="RS" direction="in"/>
<pin name="CANL"/>
<pin name="CANH"/>
<pin name="VREF" direction="out"/>
<pin name="RXD" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="UDA1320">
<pin name="BCK" direction="in"/>
<pin name="WS" direction="in"/>
<pin name="DATAI" direction="in"/>
<pin name="SYSCLK" direction="in"/>
<pin name="VOUTL" direction="out"/>
<pin name="VOUTR" direction="out"/>
<pin name="VREFDAC" direction="in"/>
<pin name="APPSEL" direction="in"/>
<pin name="APPL0" direction="in"/>
<pin name="APPL1" direction="in"/>
<pin name="APPL2" direction="in"/>
<pin name="APPL3" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSSD" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
</symbol>
<symbol name="UDA1360T">
<pin name="BCK" direction="in"/>
<pin name="WS" direction="in"/>
<pin name="DATAO" direction="in"/>
<pin name="SYSCLK" direction="in"/>
<pin name="VINL" direction="in"/>
<pin name="VINR" direction="in"/>
<pin name="VREF" direction="in"/>
<pin name="SFOR" direction="in"/>
<pin name="FSEL" direction="in"/>
<pin name="PWON" direction="in"/>
<pin name="VSSA" direction="pwr"/>
<pin name="VSSD" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VREFP" direction="in"/>
<pin name="VREFN" direction="in"/>
</symbol>
<symbol name="PFC8583">
<pin name="A0" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PCF8584">
<pin name="A0" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="!IACK" direction="in"/>
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
</symbol>
<symbol name="UAA3220TS">
<pin name="MGND" direction="pas"/>
<pin name="MIXIN" direction="pas"/>
<pin name="FA" direction="pas"/>
<pin name="VCCI" direction="pwr"/>
<pin name="LIN" direction="pas"/>
<pin name="LFB" direction="pas"/>
<pin name="RSSI" direction="pas"/>
<pin name="CPC" direction="pas"/>
<pin name="CPB" direction="pas"/>
<pin name="CPA" direction="pas"/>
<pin name="DATA" direction="pas"/>
<pin name="CGND" direction="pwr"/>
<pin name="OGND" direction="pwr"/>
<pin name="OSE" direction="pas"/>
<pin name="OSB" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="OSC" direction="oc"/>
<pin name="TEM" direction="pas"/>
<pin name="TN" direction="oc"/>
<pin name="TP" direction="oc"/>
<pin name="PWD" direction="pas"/>
<pin name="DEMO1" direction="pas"/>
<pin name="DEMO2" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="80C52">
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="RESET"/>
<pin name="P30"/>
<pin name="VSS@3"/>
<pin name="P31"/>
<pin name="P32"/>
<pin name="P33"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="P36"/>
<pin name="P37"/>
<pin name="X2" direction="out"/>
<pin name="X1" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="NC"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="VSS@2"/>
<pin name="!EA" direction="in"/>
<pin name="P07"/>
<pin name="P06"/>
<pin name="P05"/>
<pin name="P04"/>
<pin name="P03"/>
<pin name="P02"/>
<pin name="P01"/>
<pin name="P00"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS@1"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
</symbol>
<symbol name="80C52-PLCC44">
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="RESET"/>
<pin name="P30"/>
<pin name="NC@1"/>
<pin name="P31"/>
<pin name="P32"/>
<pin name="P33"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="P36"/>
<pin name="P37"/>
<pin name="X2" direction="out"/>
<pin name="X1" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="NC"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="NC@2"/>
<pin name="!EA" direction="in"/>
<pin name="P07"/>
<pin name="P06"/>
<pin name="P05"/>
<pin name="P04"/>
<pin name="P03"/>
<pin name="P02"/>
<pin name="P01"/>
<pin name="P00"/>
<pin name="VDD" direction="pwr"/>
<pin name="NC@3"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
</symbol>
<symbol name="80C52DIL40">
<pin name="P15"/>
<pin name="P16"/>
<pin name="P17"/>
<pin name="RESET"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="P32"/>
<pin name="P33"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="P36"/>
<pin name="P37"/>
<pin name="X2" direction="out"/>
<pin name="X1" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="P20"/>
<pin name="P21"/>
<pin name="P22"/>
<pin name="P23"/>
<pin name="P24"/>
<pin name="P25"/>
<pin name="P26"/>
<pin name="P27"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="P07"/>
<pin name="P06"/>
<pin name="P05"/>
<pin name="P04"/>
<pin name="P03"/>
<pin name="P02"/>
<pin name="P01"/>
<pin name="P00"/>
<pin name="VDD" direction="pwr"/>
<pin name="P10"/>
<pin name="P11"/>
<pin name="P12"/>
<pin name="P13"/>
<pin name="P14"/>
</symbol>
<symbol name="PWR">
<pin name="VCC" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="CGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="8XC592">
<pin name="EA" direction="in" function="dot"/>
<pin name="P0.0/D0"/>
<pin name="P0.1/D1"/>
<pin name="P0.2/D2"/>
<pin name="P0.3/D3"/>
<pin name="P0.4/D4"/>
<pin name="P0.5/D5"/>
<pin name="P0.6/D6"/>
<pin name="P0.7/D7"/>
<pin name="P5.0/AN0"/>
<pin name="P5.1/AN1"/>
<pin name="P5.2/AN2"/>
<pin name="P5.3/AN3"/>
<pin name="P5.4/AN4"/>
<pin name="P5.5/AN5"/>
<pin name="P5.6/AN6"/>
<pin name="P5.7/AN7"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out" function="dot"/>
<pin name="VAREF"/>
<pin name="VAGND"/>
<pin name="P4.3"/>
<pin name="P2.0/A8"/>
<pin name="P4.2"/>
<pin name="P4.1"/>
<pin name="P4.0"/>
<pin name="P2.1/A9"/>
<pin name="P2.2/A10"/>
<pin name="P2.3/A11"/>
<pin name="P2.4/A12"/>
<pin name="P2.5/A13"/>
<pin name="P2.6/A14"/>
<pin name="P2.7/A15"/>
<pin name="INT2"/>
<pin name="INT3"/>
<pin name="INT4"/>
<pin name="INT5"/>
<pin name="T2"/>
<pin name="RT2"/>
<pin name="CTX0"/>
<pin name="CTX1"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2" function="dot"/>
<pin name="P3.3" function="dot"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR" function="dot"/>
<pin name="P3.7/RD" function="dot"/>
<pin name="REF"/>
<pin name="CRX0"/>
<pin name="CRX1"/>
<pin name="STADC"/>
<pin name="PWM0"/>
<pin name="PWM1"/>
<pin name="/EW" function="dot"/>
</symbol>
<symbol name="PWR5+2">
<pin name="VDD" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="VREF" direction="pwr"/>
<pin name="AVREF-" direction="pwr"/>
</symbol>
<symbol name="8XC752">
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VPP" direction="pwr"/>
</symbol>
<symbol name="PWR2">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="8XC751">
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="VPP" direction="pwr"/>
</symbol>
<symbol name="8XC748">
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="X1" direction="in" function="clk"/>
<pin name="X2" direction="in" function="clk"/>
<pin name="VPP" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="ASEL" direction="out"/>
<pin name="OE-PGM" direction="in"/>
</symbol>
<symbol name="8XC576">
<pin name="EA" direction="in" function="dot"/>
<pin name="P0.0/D0"/>
<pin name="P0.1/D1"/>
<pin name="P0.2/D2"/>
<pin name="P0.3/D3"/>
<pin name="P0.4/D4"/>
<pin name="P0.5/D5"/>
<pin name="P0.6/D6"/>
<pin name="P0.7/D7"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out" function="dot"/>
<pin name="P2.0/A8"/>
<pin name="P2.1/A9"/>
<pin name="P2.2/A10"/>
<pin name="P2.3/A11"/>
<pin name="P2.4/A12"/>
<pin name="P2.5/A13"/>
<pin name="P2.6/A14"/>
<pin name="P2.7/A15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2" function="dot"/>
<pin name="P3.3" function="dot"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR" function="dot"/>
<pin name="P3.7/RD" function="dot"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
</symbol>
<symbol name="PWRA">
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="8XC598">
<pin name="EA" direction="in" function="dot"/>
<pin name="P0.0/D0"/>
<pin name="P0.1/D1"/>
<pin name="P0.2/D2"/>
<pin name="P0.3/D3"/>
<pin name="P0.4/D4"/>
<pin name="P0.5/D5"/>
<pin name="P0.6/D6"/>
<pin name="P0.7/D7"/>
<pin name="P5.0/AN0"/>
<pin name="P5.1/AN1"/>
<pin name="P5.2/AN2"/>
<pin name="P5.3/AN3"/>
<pin name="P5.4/AN4"/>
<pin name="P5.5/AN5"/>
<pin name="P5.6/AN6"/>
<pin name="P5.7/AN7"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out" function="dot"/>
<pin name="VAREF"/>
<pin name="VAGND"/>
<pin name="P4.3"/>
<pin name="P2.0/A8"/>
<pin name="P4.2"/>
<pin name="P4.1"/>
<pin name="P4.0"/>
<pin name="P2.1/A9"/>
<pin name="P2.2/A10"/>
<pin name="P2.3/A11"/>
<pin name="P2.4/A12"/>
<pin name="P2.5/A13"/>
<pin name="P2.6/A14"/>
<pin name="P2.7/A15"/>
<pin name="INT2"/>
<pin name="INT3"/>
<pin name="INT4"/>
<pin name="INT5"/>
<pin name="T2"/>
<pin name="RT2"/>
<pin name="CTX0"/>
<pin name="CTX1"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2" function="dot"/>
<pin name="P3.3" function="dot"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR" function="dot"/>
<pin name="P3.7/RD" function="dot"/>
<pin name="REF"/>
<pin name="CRX0"/>
<pin name="CRX1"/>
<pin name="STADC"/>
<pin name="PWM0"/>
<pin name="PWM1"/>
<pin name="/EW" function="dot"/>
</symbol>
<symbol name="8XC562">
<pin name="EA" direction="in" function="dot"/>
<pin name="P0.0/D0"/>
<pin name="P0.1/D1"/>
<pin name="P0.2/D2"/>
<pin name="P0.3/D3"/>
<pin name="P0.4/D4"/>
<pin name="P0.5/D5"/>
<pin name="P0.6/D6"/>
<pin name="P0.7/D7"/>
<pin name="P5.0/ADC0"/>
<pin name="P5.1/ADC1"/>
<pin name="P5.2/ADC2"/>
<pin name="P5.3/ADC3"/>
<pin name="P5.4/ADC4"/>
<pin name="P5.5/ADC5"/>
<pin name="P5.6/ADC6"/>
<pin name="P5.7/ADC7"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out" function="dot"/>
<pin name="P4.0/CMSR0"/>
<pin name="P2.0/A8" direction="out"/>
<pin name="P4.1/CMSR1"/>
<pin name="P4.2/CMSR2"/>
<pin name="P4.3/CMSR3"/>
<pin name="P2.1/A9" direction="out"/>
<pin name="P2.2/A10" direction="out"/>
<pin name="P2.3/A11" direction="out"/>
<pin name="P2.4/A12" direction="out"/>
<pin name="P2.5/A13" direction="out"/>
<pin name="P2.6/A14" direction="out"/>
<pin name="P2.7/A15" direction="out"/>
<pin name="P1.0/CT0I"/>
<pin name="P1.1/CT1I"/>
<pin name="P1.2/CT2I"/>
<pin name="P1.3/CT3I"/>
<pin name="P1.4/T2"/>
<pin name="P1.5/RT2"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P4.4/CMSR4"/>
<pin name="P4.5/CMSR5"/>
<pin name="P4.6/CMT0"/>
<pin name="P4.7/CMT1"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2" function="dot"/>
<pin name="P3.3" function="dot"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR" function="dot"/>
<pin name="P3.7/RD" function="dot"/>
<pin name="STADC"/>
<pin name="PWM0"/>
<pin name="PWM1"/>
<pin name="/EW" function="dot"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
</symbol>
<symbol name="8XC558">
<pin name="EA" direction="in" function="dot"/>
<pin name="P0.0/D0"/>
<pin name="P0.1/D1"/>
<pin name="P0.2/D2"/>
<pin name="P0.3/D3"/>
<pin name="P0.4/D4"/>
<pin name="P0.5/D5"/>
<pin name="P0.6/D6"/>
<pin name="P0.7/D7"/>
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.4"/>
<pin name="P5.5"/>
<pin name="P5.6"/>
<pin name="P5.7"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="RST" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out" function="dot"/>
<pin name="P4.3"/>
<pin name="P2.0/A8" direction="out"/>
<pin name="P4.2"/>
<pin name="P4.1"/>
<pin name="P4.0"/>
<pin name="P2.1/A9" direction="out"/>
<pin name="P2.2/A10" direction="out"/>
<pin name="P2.3/A11" direction="out"/>
<pin name="P2.4/A12" direction="out"/>
<pin name="P2.5/A13" direction="out"/>
<pin name="P2.6/A14" direction="out"/>
<pin name="P2.7/A15" direction="out"/>
<pin name="P1.0/CT0I"/>
<pin name="P1.1/CT1I"/>
<pin name="P1.2/CT2I"/>
<pin name="P1.3/CT3I"/>
<pin name="P1.4/T2"/>
<pin name="P1.5/RT2"/>
<pin name="P1.6/SCL"/>
<pin name="P1.7/SDA"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2" function="dot"/>
<pin name="P3.3" function="dot"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR" function="dot"/>
<pin name="P3.7/RD" function="dot"/>
<pin name="STADC"/>
<pin name="PWM0"/>
<pin name="PWM1"/>
<pin name="/EW" function="dot"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
</symbol>
<symbol name="8XCE559">
<pin name="EA1" direction="in" function="dot"/>
<pin name="P0.0/D1"/>
<pin name="P0.1/D2"/>
<pin name="P0.2/D1"/>
<pin name="P0.3/D1"/>
<pin name="P0.4/D1"/>
<pin name="P0.5/D1"/>
<pin name="P0.6/D1"/>
<pin name="P0.7/D1"/>
<pin name="P5.8"/>
<pin name="P5.9"/>
<pin name="P5.10"/>
<pin name="P5.11"/>
<pin name="P5.12"/>
<pin name="P5.13"/>
<pin name="P5.14"/>
<pin name="P5.15"/>
<pin name="XTAL3" direction="in" function="clk"/>
<pin name="XTAL4" direction="in" function="clk"/>
<pin name="RST1" direction="in"/>
<pin name="ALE1" direction="out"/>
<pin name="PSEN1" direction="out" function="dot"/>
<pin name="P4.8"/>
<pin name="P2.0/A1" direction="out"/>
<pin name="P4.9"/>
<pin name="P4.10"/>
<pin name="P4.11"/>
<pin name="P2.1/A1" direction="out"/>
<pin name="P2.2/A1" direction="out"/>
<pin name="P2.3/A1" direction="out"/>
<pin name="P2.4/A1" direction="out"/>
<pin name="P2.5/A1" direction="out"/>
<pin name="P2.6/A1" direction="out"/>
<pin name="P2.7/A1" direction="out"/>
<pin name="P1.0/CT0I1"/>
<pin name="P1.1/CT1I1"/>
<pin name="P1.2/CT2I1"/>
<pin name="P1.3/CT3I1"/>
<pin name="P1.4/T1"/>
<pin name="P1.5/RT1"/>
<pin name="P1.6/SCL1"/>
<pin name="P1.7/SDA1"/>
<pin name="P4.12"/>
<pin name="P4.13"/>
<pin name="P4.14"/>
<pin name="P4.15"/>
<pin name="P3.4"/>
<pin name="P3.5"/>
<pin name="P3.6" function="dot"/>
<pin name="P3.7" function="dot"/>
<pin name="P3.4/T1"/>
<pin name="P3.5/T2"/>
<pin name="P3.6/WR1" function="dot"/>
<pin name="P3.7/RD1" function="dot"/>
<pin name="STADC1"/>
<pin name="PWM2"/>
<pin name="PWM3"/>
<pin name="/EW1" function="dot"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
</symbol>
<symbol name="NC5">
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
</symbol>
<symbol name="PWR5">
<pin name="VCC@0" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
</symbol>
<symbol name="PWRC">
<pin name="CVCC" direction="pwr"/>
<pin name="CGND" direction="pwr"/>
</symbol>
<symbol name="82C200">
<pin name="AD0" direction="hiz"/>
<pin name="AD1" direction="hiz"/>
<pin name="AD2" direction="hiz"/>
<pin name="AD3" direction="hiz"/>
<pin name="AD4" direction="hiz"/>
<pin name="AD5" direction="hiz"/>
<pin name="AD6" direction="hiz"/>
<pin name="AD7" direction="hiz"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="MODE" direction="in"/>
<pin name="/RST" direction="in" function="dot"/>
<pin name="/INT" direction="out" function="dot"/>
<pin name="ALE"/>
<pin name="/CS" direction="in" function="dot"/>
<pin name="/RD" direction="in" function="dot"/>
<pin name="/WR" direction="in" function="dot"/>
<pin name="CLK_OUT" direction="out"/>
<pin name="TX0" direction="out"/>
<pin name="TX1" direction="out"/>
<pin name="RX0" direction="in"/>
<pin name="RX1" direction="in"/>
</symbol>
<symbol name="PWRCAN">
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@0" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="PWR4">
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
</symbol>
<symbol name="82B715">
<pin name="LX"/>
<pin name="LY"/>
<pin name="SX"/>
<pin name="SY"/>
</symbol>
<symbol name="NC2">
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
</symbol>
<symbol name="NC1">
<pin name="NC"/>
</symbol>
<symbol name="VDD">
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="PCA9555">
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!INT" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="I/O0.0"/>
<pin name="I/O0.1"/>
<pin name="I/O0.2"/>
<pin name="I/O0.3"/>
<pin name="I/O0.4"/>
<pin name="I/O0.5"/>
<pin name="I/O0.6"/>
<pin name="I/O0.7"/>
<pin name="I/O1.0"/>
<pin name="I/O1.1"/>
<pin name="I/O1.2"/>
<pin name="I/O1.3"/>
<pin name="I/O1.4"/>
<pin name="I/O1.5"/>
<pin name="I/O1.6"/>
<pin name="I/O1.7"/>
</symbol>
<symbol name="PN531">
<pin name="DVDD" direction="in"/>
<pin name="DVSS" direction="pwr"/>
<pin name="P32_INT0"/>
<pin name="P33_INT1"/>
<pin name="!RSTOUT"/>
<pin name="IRQ" direction="out"/>
<pin name="SCK"/>
<pin name="MISO"/>
<pin name="MOSI"/>
<pin name="NSS"/>
<pin name="P30"/>
<pin name="P31"/>
<pin name="P34"/>
<pin name="P35"/>
<pin name="OSC2IN" direction="in"/>
<pin name="VBUS" direction="in"/>
<pin name="DELATT" direction="out"/>
<pin name="TESTEN" direction="in"/>
<pin name="OSC2OUT" direction="out"/>
<pin name="PVDD" direction="pwr"/>
<pin name="SVDD" direction="pwr"/>
<pin name="!RSTPD" direction="in"/>
<pin name="OSCOUT" direction="out"/>
<pin name="OSCIN" direction="in"/>
<pin name="TVDD" direction="pwr"/>
<pin name="TVSS1" direction="pwr"/>
<pin name="TX1" direction="out"/>
<pin name="TX2" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="RX" direction="in"/>
<pin name="VMID" direction="pwr"/>
<pin name="AUX1" direction="out"/>
<pin name="AUX2" direction="out"/>
<pin name="SIGOUT" direction="out"/>
<pin name="SIGIN" direction="in"/>
<pin name="LOADMOD" direction="out"/>
<pin name="TVSS2" direction="pwr"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="TEA5764HN">
<pin name="LOOPSW" direction="in"/>
<pin name="CPOUT" direction="in"/>
<pin name="LO1" direction="in"/>
<pin name="LO2" direction="in"/>
<pin name="CD1" direction="in"/>
<pin name="PILLP" direction="in"/>
<pin name="SWPORT" direction="out"/>
<pin name="BUSENBABLE" direction="in"/>
<pin name="VREFDIG" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="GNDD" direction="pwr"/>
<pin name="GNDD@1" direction="pwr"/>
<pin name="VCCD" direction="pwr"/>
<pin name="CD2/INTCON3" direction="in"/>
<pin name="INTCON2" direction="in"/>
<pin name="GNDD@2" direction="pwr"/>
<pin name="INTX" direction="out"/>
<pin name="INTCON1" direction="in"/>
<pin name="TMUTE" direction="in"/>
<pin name="VAFR" direction="out"/>
<pin name="VAFL" direction="out"/>
<pin name="MPXOUT" direction="out"/>
<pin name="GNDD@3" direction="pwr"/>
<pin name="GNDA" direction="in"/>
<pin name="FREQIN" direction="in"/>
<pin name="XTAL" direction="in"/>
<pin name="VCCA" direction="in"/>
<pin name="CD3" direction="in"/>
<pin name="RFIN1" direction="in"/>
<pin name="RFIN2" direction="in"/>
<pin name="GNDRF" direction="in"/>
<pin name="CAGC" direction="in"/>
<pin name="MPXIN" direction="in"/>
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="P98LPC935">
<pin name="AD03/DAC0/P2.0"/>
<pin name="AD02/P2.1"/>
<pin name="AD01/P2.0"/>
<pin name="AD00/P1.7"/>
<pin name="OCB/P1.6"/>
<pin name="VSS"/>
<pin name="XTAL1/P3.1"/>
<pin name="CLKOUT/XTAL2/P3.0"/>
<pin name="!INT1/P1.4"/>
<pin name="SDA/!INT0/P1.2"/>
<pin name="SCL/T0/P1.2"/>
<pin name="MOSI/P2.2"/>
<pin name="MISO/P2.3"/>
<pin name="P2.4/!SS"/>
<pin name="P2.5/SPICLK"/>
<pin name="P1.1/RXD"/>
<pin name="P1.0/TXD"/>
<pin name="P0.7/T1"/>
<pin name="P0.6/CMP1"/>
<pin name="VDD"/>
<pin name="P0.5/CMPREF"/>
<pin name="P0.4/CIN1A/DAC1/AD13"/>
<pin name="P0.3/CIN1B/AD12"/>
<pin name="P0.2/CIN2A/AD11"/>
<pin name="P0.1/CIN2B/AD10"/>
<pin name="P2.6/OCA"/>
<pin name="P2.7/ICA"/>
<pin name="!RST/P1.5"/>
</symbol>
<symbol name="PCA9505">
<pin name="A0" direction="in"/>
<pin name="!INT" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="IO0_0"/>
<pin name="!OE" direction="in"/>
<pin name="IO0_1"/>
<pin name="IO0_2"/>
<pin name="IO0_3"/>
<pin name="IO0_4"/>
<pin name="IO0_5"/>
<pin name="IO0_6"/>
<pin name="IO0_7"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="IO1_0"/>
<pin name="IO1_1"/>
<pin name="IO1_2"/>
<pin name="IO1_3"/>
<pin name="IO1_4"/>
<pin name="IO1_5"/>
<pin name="IO1_6"/>
<pin name="IO1_7"/>
<pin name="IO2_0"/>
<pin name="IO2_1"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="IO2_2"/>
<pin name="IO2_3"/>
<pin name="IO2_4"/>
<pin name="IO2_5"/>
<pin name="IO2_6"/>
<pin name="IO2_7"/>
<pin name="IO3_0"/>
<pin name="IO3_1"/>
<pin name="IO3_2"/>
<pin name="IO3_3"/>
<pin name="IO3_4"/>
<pin name="IO3_5"/>
<pin name="IO3_6"/>
<pin name="IO3_7"/>
<pin name="IO4_0"/>
<pin name="IO4_1"/>
<pin name="IO4_2"/>
<pin name="IO4_3"/>
<pin name="IO4_4"/>
<pin name="IO4_5"/>
<pin name="IO4_6"/>
<pin name="IO4_7"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
</symbol>
<symbol name="PCA9506">
<pin name="A0" direction="in"/>
<pin name="!INT" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="IO0_0"/>
<pin name="!OE" direction="in"/>
<pin name="IO0_1"/>
<pin name="IO0_2"/>
<pin name="IO0_3"/>
<pin name="IO0_4"/>
<pin name="IO0_5"/>
<pin name="IO0_6"/>
<pin name="IO0_7"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="IO1_0"/>
<pin name="IO1_1"/>
<pin name="IO1_2"/>
<pin name="IO1_3"/>
<pin name="IO1_4"/>
<pin name="IO1_5"/>
<pin name="IO1_6"/>
<pin name="IO1_7"/>
<pin name="IO2_0"/>
<pin name="IO2_1"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="IO2_2"/>
<pin name="IO2_3"/>
<pin name="IO2_4"/>
<pin name="IO2_5"/>
<pin name="IO2_6"/>
<pin name="IO2_7"/>
<pin name="IO3_0"/>
<pin name="IO3_1"/>
<pin name="IO3_2"/>
<pin name="IO3_3"/>
<pin name="IO3_4"/>
<pin name="IO3_5"/>
<pin name="IO3_6"/>
<pin name="IO3_7"/>
<pin name="IO4_0"/>
<pin name="IO4_1"/>
<pin name="IO4_2"/>
<pin name="IO4_3"/>
<pin name="IO4_4"/>
<pin name="IO4_5"/>
<pin name="IO4_6"/>
<pin name="IO4_7"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
</symbol>
<symbol name="PCA9534">
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="!INT" direction="oc"/>
<pin name="IO0"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
</symbol>
<symbol name="LPC1102">
<pin name="VDD" direction="pwr"/>
<pin name="PIO0_8/MISO/CT16B0_MAT0"/>
<pin name="PIO0_9/MOSI/CT16B0_MAT1"/>
<pin name="SWCLK/PIO0_10/SCK/CT16B0_MAT2"/>
<pin name="VSS" direction="pwr"/>
<pin name="XTALIN" direction="in"/>
<pin name="R/PIO1_0/AD1/CT32B1_CAP0"/>
<pin name="R/PIO0_11/AD0/CT32B0_MAT3"/>
<pin name="RESET/PIO0_0"/>
<pin name="PIO1_6/RXD/CT32B0_MAT0"/>
<pin name="R/PIO1_2/AD3/CT32B1_MAT1"/>
<pin name="R/PIO1_1/AD2/CT32B1_MAT0"/>
<pin name="PIO1_7/TXD/CT32B0_MAT1"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="SWDIO/PIO1_3/AD4/CT32B1_MAT2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="P90CL301" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="P90CL301"/>
</gates>
<devices>
<device name="" package="QFP12-80">
<connects>
<connect gate="G$1" pin="A1" pad="14"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="24"/>
<connect gate="G$1" pin="A12" pad="25"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="28"/>
<connect gate="G$1" pin="A16" pad="29"/>
<connect gate="G$1" pin="A17" pad="30"/>
<connect gate="G$1" pin="A18" pad="31"/>
<connect gate="G$1" pin="A2" pad="15"/>
<connect gate="G$1" pin="A3" pad="16"/>
<connect gate="G$1" pin="A4" pad="17"/>
<connect gate="G$1" pin="A5" pad="18"/>
<connect gate="G$1" pin="A6" pad="19"/>
<connect gate="G$1" pin="A7" pad="20"/>
<connect gate="G$1" pin="A8" pad="21"/>
<connect gate="G$1" pin="A9" pad="22"/>
<connect gate="G$1" pin="AS" pad="1"/>
<connect gate="G$1" pin="BSIZE" pad="58"/>
<connect gate="G$1" pin="CS0/FC0" pad="44"/>
<connect gate="G$1" pin="CS1/FC1" pad="43"/>
<connect gate="G$1" pin="CS2/FC2" pad="42"/>
<connect gate="G$1" pin="CS3/ALE" pad="41"/>
<connect gate="G$1" pin="CS4/RD" pad="40"/>
<connect gate="G$1" pin="CS5/WR" pad="39"/>
<connect gate="G$1" pin="CS6/A23" pad="37"/>
<connect gate="G$1" pin="CSBT/ONCE" pad="38"/>
<connect gate="G$1" pin="D0" pad="9"/>
<connect gate="G$1" pin="D1" pad="8"/>
<connect gate="G$1" pin="D10/P2" pad="75"/>
<connect gate="G$1" pin="D11/P3" pad="74"/>
<connect gate="G$1" pin="D12/P4" pad="73"/>
<connect gate="G$1" pin="D13/P5" pad="72"/>
<connect gate="G$1" pin="D14/P6" pad="71"/>
<connect gate="G$1" pin="D15/P7" pad="70"/>
<connect gate="G$1" pin="D2" pad="7"/>
<connect gate="G$1" pin="D3" pad="6"/>
<connect gate="G$1" pin="D4" pad="5"/>
<connect gate="G$1" pin="D5" pad="4"/>
<connect gate="G$1" pin="D6" pad="3"/>
<connect gate="G$1" pin="D7" pad="2"/>
<connect gate="G$1" pin="D8/P0" pad="77"/>
<connect gate="G$1" pin="D9/P1" pad="76"/>
<connect gate="G$1" pin="DTACK" pad="78"/>
<connect gate="G$1" pin="HALT" pad="68"/>
<connect gate="G$1" pin="LDS/DS" pad="80"/>
<connect gate="G$1" pin="P10/SCL" pad="56"/>
<connect gate="G$1" pin="P11/SDA" pad="57"/>
<connect gate="G$1" pin="P12/ADC0" pad="64"/>
<connect gate="G$1" pin="P13/ADC1" pad="63"/>
<connect gate="G$1" pin="P14/ADC2" pad="62"/>
<connect gate="G$1" pin="P15/ADC3" pad="60"/>
<connect gate="G$1" pin="P8/PWM0" pad="54"/>
<connect gate="G$1" pin="P9/PWM1" pad="55"/>
<connect gate="G$1" pin="PCS0/A19" pad="33"/>
<connect gate="G$1" pin="PCS1/A20" pad="34"/>
<connect gate="G$1" pin="PCS2/A21" pad="35"/>
<connect gate="G$1" pin="PCS3/A22" pad="36"/>
<connect gate="G$1" pin="RESET" pad="67"/>
<connect gate="G$1" pin="RESETIN" pad="66"/>
<connect gate="G$1" pin="SP0/INT0/" pad="53"/>
<connect gate="G$1" pin="SP1/INT1/" pad="52"/>
<connect gate="G$1" pin="SP2/INT2/" pad="50"/>
<connect gate="G$1" pin="SP3/INT3/" pad="49"/>
<connect gate="G$1" pin="SP4/INT4" pad="48"/>
<connect gate="G$1" pin="SP5/INT5" pad="47"/>
<connect gate="G$1" pin="SP6/INT6" pad="46"/>
<connect gate="G$1" pin="SP7/NMIN" pad="45"/>
<connect gate="G$1" pin="TROM_R/W" pad="79"/>
<connect gate="G$1" pin="UDS/A0" pad="13"/>
<connect gate="G$1" pin="VDD" pad="69"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VDD@2" pad="10"/>
<connect gate="G$1" pin="VDDA" pad="59"/>
<connect gate="G$1" pin="VREF" pad="61"/>
<connect gate="G$1" pin="VSS" pad="51"/>
<connect gate="G$1" pin="VSS@1" pad="12"/>
<connect gate="G$1" pin="VSSA" pad="65"/>
<connect gate="G$1" pin="XTAL1" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C552" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C552"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="A08-P2.0" pad="39"/>
<connect gate="G$1" pin="A09-P2.1" pad="40"/>
<connect gate="G$1" pin="A10-P2.2" pad="41"/>
<connect gate="G$1" pin="A11-P2.3" pad="42"/>
<connect gate="G$1" pin="A12-P2.4" pad="43"/>
<connect gate="G$1" pin="A13-P2.5" pad="44"/>
<connect gate="G$1" pin="A14-P2.6" pad="45"/>
<connect gate="G$1" pin="A15-P2.7" pad="46"/>
<connect gate="G$1" pin="AD0-P0.0" pad="57"/>
<connect gate="G$1" pin="AD1-P0.1" pad="56"/>
<connect gate="G$1" pin="AD2-P0.2" pad="55"/>
<connect gate="G$1" pin="AD3-P0.3" pad="54"/>
<connect gate="G$1" pin="AD4-P0.4" pad="53"/>
<connect gate="G$1" pin="AD5-P0.5" pad="52"/>
<connect gate="G$1" pin="AD6-P0.6" pad="51"/>
<connect gate="G$1" pin="AD7-P0.7" pad="50"/>
<connect gate="G$1" pin="ALE-PROG/" pad="48"/>
<connect gate="G$1" pin="AVDD" pad="61"/>
<connect gate="G$1" pin="AVREF+" pad="59"/>
<connect gate="G$1" pin="AVREF-" pad="58"/>
<connect gate="G$1" pin="AVSS" pad="60"/>
<connect gate="G$1" pin="CSL-P1.6" pad="22"/>
<connect gate="G$1" pin="CT0I-P1.0" pad="16"/>
<connect gate="G$1" pin="CT1I-P1.1" pad="17"/>
<connect gate="G$1" pin="CT2I-P1.2" pad="18"/>
<connect gate="G$1" pin="CT3I-P1.3" pad="19"/>
<connect gate="G$1" pin="EA/VPP" pad="49"/>
<connect gate="G$1" pin="EW/" pad="6"/>
<connect gate="G$1" pin="NC1" pad="32"/>
<connect gate="G$1" pin="NC2" pad="33"/>
<connect gate="G$1" pin="NC3" pad="38"/>
<connect gate="G$1" pin="P3.0-RXD" pad="24"/>
<connect gate="G$1" pin="P3.1-TXD" pad="25"/>
<connect gate="G$1" pin="P3.2-INT0/" pad="26"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="27"/>
<connect gate="G$1" pin="P3.4-T0" pad="28"/>
<connect gate="G$1" pin="P3.5-T1" pad="29"/>
<connect gate="G$1" pin="P3.6-WR/" pad="30"/>
<connect gate="G$1" pin="P3.7-RD/" pad="31"/>
<connect gate="G$1" pin="P4.0-CMSR0" pad="7"/>
<connect gate="G$1" pin="P4.1-CMSR1" pad="8"/>
<connect gate="G$1" pin="P4.2-CMSR2" pad="9"/>
<connect gate="G$1" pin="P4.3-CMSR3" pad="10"/>
<connect gate="G$1" pin="P4.4-CMSR4" pad="11"/>
<connect gate="G$1" pin="P4.5-CMSR5" pad="12"/>
<connect gate="G$1" pin="P4.6-CMT0" pad="13"/>
<connect gate="G$1" pin="P4.7-CMT1" pad="14"/>
<connect gate="G$1" pin="P5.0-ADC0" pad="1"/>
<connect gate="G$1" pin="P5.1-ADC1" pad="68"/>
<connect gate="G$1" pin="P5.2-ADC2" pad="67"/>
<connect gate="G$1" pin="P5.3-ADC3" pad="66"/>
<connect gate="G$1" pin="P5.4-ADC4" pad="65"/>
<connect gate="G$1" pin="P5.5-ADC5" pad="64"/>
<connect gate="G$1" pin="P5.6-ADC6" pad="63"/>
<connect gate="G$1" pin="P5.7-ADC7" pad="62"/>
<connect gate="G$1" pin="PSEN/" pad="47"/>
<connect gate="G$1" pin="PWM0/" pad="4"/>
<connect gate="G$1" pin="PWM1/" pad="5"/>
<connect gate="G$1" pin="RST" pad="15"/>
<connect gate="G$1" pin="RT2-P1.5" pad="21"/>
<connect gate="G$1" pin="SDA-P1.7" pad="23"/>
<connect gate="G$1" pin="STADC" pad="3"/>
<connect gate="G$1" pin="T2-P1.4" pad="20"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="36"/>
<connect gate="G$1" pin="VSS@1" pad="37"/>
<connect gate="G$1" pin="XTAL1" pad="35"/>
<connect gate="G$1" pin="XTAL2" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C552IBA/08,512"/>
<attribute name="OC_FARNELL" value="1831232"/>
<attribute name="OC_NEWARK" value="70R8448"/>
</technology>
</technologies>
</device>
<device name="N-S" package="PLCC-S68">
<connects>
<connect gate="G$1" pin="A08-P2.0" pad="39"/>
<connect gate="G$1" pin="A09-P2.1" pad="40"/>
<connect gate="G$1" pin="A10-P2.2" pad="41"/>
<connect gate="G$1" pin="A11-P2.3" pad="42"/>
<connect gate="G$1" pin="A12-P2.4" pad="43"/>
<connect gate="G$1" pin="A13-P2.5" pad="44"/>
<connect gate="G$1" pin="A14-P2.6" pad="45"/>
<connect gate="G$1" pin="A15-P2.7" pad="46"/>
<connect gate="G$1" pin="AD0-P0.0" pad="57"/>
<connect gate="G$1" pin="AD1-P0.1" pad="56"/>
<connect gate="G$1" pin="AD2-P0.2" pad="55"/>
<connect gate="G$1" pin="AD3-P0.3" pad="54"/>
<connect gate="G$1" pin="AD4-P0.4" pad="53"/>
<connect gate="G$1" pin="AD5-P0.5" pad="52"/>
<connect gate="G$1" pin="AD6-P0.6" pad="51"/>
<connect gate="G$1" pin="AD7-P0.7" pad="50"/>
<connect gate="G$1" pin="ALE-PROG/" pad="48"/>
<connect gate="G$1" pin="AVDD" pad="61"/>
<connect gate="G$1" pin="AVREF+" pad="59"/>
<connect gate="G$1" pin="AVREF-" pad="58"/>
<connect gate="G$1" pin="AVSS" pad="60"/>
<connect gate="G$1" pin="CSL-P1.6" pad="22"/>
<connect gate="G$1" pin="CT0I-P1.0" pad="16"/>
<connect gate="G$1" pin="CT1I-P1.1" pad="17"/>
<connect gate="G$1" pin="CT2I-P1.2" pad="18"/>
<connect gate="G$1" pin="CT3I-P1.3" pad="19"/>
<connect gate="G$1" pin="EA/VPP" pad="49"/>
<connect gate="G$1" pin="EW/" pad="6"/>
<connect gate="G$1" pin="NC1" pad="32"/>
<connect gate="G$1" pin="NC2" pad="33"/>
<connect gate="G$1" pin="NC3" pad="38"/>
<connect gate="G$1" pin="P3.0-RXD" pad="24"/>
<connect gate="G$1" pin="P3.1-TXD" pad="25"/>
<connect gate="G$1" pin="P3.2-INT0/" pad="26"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="27"/>
<connect gate="G$1" pin="P3.4-T0" pad="28"/>
<connect gate="G$1" pin="P3.5-T1" pad="29"/>
<connect gate="G$1" pin="P3.6-WR/" pad="30"/>
<connect gate="G$1" pin="P3.7-RD/" pad="31"/>
<connect gate="G$1" pin="P4.0-CMSR0" pad="7"/>
<connect gate="G$1" pin="P4.1-CMSR1" pad="8"/>
<connect gate="G$1" pin="P4.2-CMSR2" pad="9"/>
<connect gate="G$1" pin="P4.3-CMSR3" pad="10"/>
<connect gate="G$1" pin="P4.4-CMSR4" pad="11"/>
<connect gate="G$1" pin="P4.5-CMSR5" pad="12"/>
<connect gate="G$1" pin="P4.6-CMT0" pad="13"/>
<connect gate="G$1" pin="P4.7-CMT1" pad="14"/>
<connect gate="G$1" pin="P5.0-ADC0" pad="1"/>
<connect gate="G$1" pin="P5.1-ADC1" pad="68"/>
<connect gate="G$1" pin="P5.2-ADC2" pad="67"/>
<connect gate="G$1" pin="P5.3-ADC3" pad="66"/>
<connect gate="G$1" pin="P5.4-ADC4" pad="65"/>
<connect gate="G$1" pin="P5.5-ADC5" pad="64"/>
<connect gate="G$1" pin="P5.6-ADC6" pad="63"/>
<connect gate="G$1" pin="P5.7-ADC7" pad="62"/>
<connect gate="G$1" pin="PSEN/" pad="47"/>
<connect gate="G$1" pin="PWM0/" pad="4"/>
<connect gate="G$1" pin="PWM1/" pad="5"/>
<connect gate="G$1" pin="RST" pad="15"/>
<connect gate="G$1" pin="RT2-P1.5" pad="21"/>
<connect gate="G$1" pin="SDA-P1.7" pad="23"/>
<connect gate="G$1" pin="STADC" pad="3"/>
<connect gate="G$1" pin="T2-P1.4" pad="20"/>
<connect gate="G$1" pin="VDD" pad="2"/>
<connect gate="G$1" pin="VSS" pad="36"/>
<connect gate="G$1" pin="VSS@1" pad="37"/>
<connect gate="G$1" pin="XTAL1" pad="35"/>
<connect gate="G$1" pin="XTAL2" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C552IBA/08,512"/>
<attribute name="OC_FARNELL" value="1831233"/>
<attribute name="OC_NEWARK" value="70R8448"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C552Q80" prefix="IC">
<description>&lt;b&gt;MICROCONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C552"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="P" symbol="VSS"/>
<gate name="NU33" symbol="NU"/>
<gate name="NU73" symbol="NU"/>
</gates>
<devices>
<device name="" package="QFP80R">
<connects>
<connect gate="G$1" pin="A08-P2.0" pad="38"/>
<connect gate="G$1" pin="A09-P2.1" pad="39"/>
<connect gate="G$1" pin="A10-P2.2" pad="40"/>
<connect gate="G$1" pin="A11-P2.3" pad="41"/>
<connect gate="G$1" pin="A12-P2.4" pad="42"/>
<connect gate="G$1" pin="A13-P2.5" pad="45"/>
<connect gate="G$1" pin="A14-P2.6" pad="46"/>
<connect gate="G$1" pin="A15-P2.7" pad="47"/>
<connect gate="G$1" pin="AD0-P0.0" pad="58"/>
<connect gate="G$1" pin="AD1-P0.1" pad="57"/>
<connect gate="G$1" pin="AD2-P0.2" pad="56"/>
<connect gate="G$1" pin="AD3-P0.3" pad="55"/>
<connect gate="G$1" pin="AD4-P0.4" pad="54"/>
<connect gate="G$1" pin="AD5-P0.5" pad="53"/>
<connect gate="G$1" pin="AD6-P0.6" pad="52"/>
<connect gate="G$1" pin="AD7-P0.7" pad="51"/>
<connect gate="G$1" pin="ALE-PROG/" pad="49"/>
<connect gate="G$1" pin="AVDD" pad="63"/>
<connect gate="G$1" pin="AVREF+" pad="60"/>
<connect gate="G$1" pin="AVREF-" pad="59"/>
<connect gate="G$1" pin="AVSS" pad="61"/>
<connect gate="G$1" pin="CSL-P1.6" pad="16"/>
<connect gate="G$1" pin="CT0I-P1.0" pad="10"/>
<connect gate="G$1" pin="CT1I-P1.1" pad="11"/>
<connect gate="G$1" pin="CT2I-P1.2" pad="12"/>
<connect gate="G$1" pin="CT3I-P1.3" pad="13"/>
<connect gate="G$1" pin="EA/VPP" pad="50"/>
<connect gate="G$1" pin="EW/" pad="77"/>
<connect gate="G$1" pin="NC1" pad="3"/>
<connect gate="G$1" pin="NC2" pad="21"/>
<connect gate="G$1" pin="NC3" pad="22"/>
<connect gate="G$1" pin="P3.0-RXD" pad="18"/>
<connect gate="G$1" pin="P3.1-TXD" pad="19"/>
<connect gate="G$1" pin="P3.2-INT0/" pad="20"/>
<connect gate="G$1" pin="P3.3-INT1/" pad="23"/>
<connect gate="G$1" pin="P3.4-T0" pad="24"/>
<connect gate="G$1" pin="P3.5-T1" pad="25"/>
<connect gate="G$1" pin="P3.6-WR/" pad="26"/>
<connect gate="G$1" pin="P3.7-RD/" pad="27"/>
<connect gate="G$1" pin="P4.0-CMSR0" pad="80"/>
<connect gate="G$1" pin="P4.1-CMSR1" pad="1"/>
<connect gate="G$1" pin="P4.2-CMSR2" pad="2"/>
<connect gate="G$1" pin="P4.3-CMSR3" pad="4"/>
<connect gate="G$1" pin="P4.4-CMSR4" pad="5"/>
<connect gate="G$1" pin="P4.5-CMSR5" pad="6"/>
<connect gate="G$1" pin="P4.6-CMT0" pad="7"/>
<connect gate="G$1" pin="P4.7-CMT1" pad="8"/>
<connect gate="G$1" pin="P5.0-ADC0" pad="71"/>
<connect gate="G$1" pin="P5.1-ADC1" pad="70"/>
<connect gate="G$1" pin="P5.2-ADC2" pad="69"/>
<connect gate="G$1" pin="P5.3-ADC3" pad="68"/>
<connect gate="G$1" pin="P5.4-ADC4" pad="67"/>
<connect gate="G$1" pin="P5.5-ADC5" pad="66"/>
<connect gate="G$1" pin="P5.6-ADC6" pad="65"/>
<connect gate="G$1" pin="P5.7-ADC7" pad="64"/>
<connect gate="G$1" pin="PSEN/" pad="48"/>
<connect gate="G$1" pin="PWM0/" pad="75"/>
<connect gate="G$1" pin="PWM1/" pad="76"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="RT2-P1.5" pad="15"/>
<connect gate="G$1" pin="SDA-P1.7" pad="17"/>
<connect gate="G$1" pin="STADC" pad="74"/>
<connect gate="G$1" pin="T2-P1.4" pad="14"/>
<connect gate="G$1" pin="VDD" pad="72"/>
<connect gate="G$1" pin="VSS" pad="34"/>
<connect gate="G$1" pin="VSS@1" pad="35"/>
<connect gate="G$1" pin="XTAL1" pad="32"/>
<connect gate="G$1" pin="XTAL2" pad="31"/>
<connect gate="NC1" pin="NC" pad="28"/>
<connect gate="NC2" pin="NC" pad="29"/>
<connect gate="NC3" pin="NC" pad="30"/>
<connect gate="NC4" pin="NC" pad="37"/>
<connect gate="NC5" pin="NC" pad="43"/>
<connect gate="NC6" pin="NC" pad="44"/>
<connect gate="NC7" pin="NC" pad="62"/>
<connect gate="NC8" pin="NC" pad="78"/>
<connect gate="NC9" pin="NC" pad="79"/>
<connect gate="NU33" pin="IC-NU" pad="33"/>
<connect gate="NU73" pin="IC-NU" pad="73"/>
<connect gate="P" pin="VSS" pad="36"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO10" prefix="_">
<description>&lt;b&gt;LOGO&lt;/b&gt; 10 mm</description>
<gates>
<gate name="-1" symbol="LOGO10"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LOGO20" prefix="_">
<description>&lt;b&gt;LOGO&lt;/b&gt; 20 mm</description>
<gates>
<gate name="-1" symbol="LOGO20"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAA1064" prefix="IC">
<description>I2C-Bus 4-digit &lt;b&gt;LED-DRIVER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SAA1064"/>
</gates>
<devices>
<device name="" package="DIL24-6">
<connects>
<connect gate="G$1" pin="ADR" pad="1"/>
<connect gate="G$1" pin="CEXT" pad="2"/>
<connect gate="G$1" pin="MX1" pad="11"/>
<connect gate="G$1" pin="MX2" pad="14"/>
<connect gate="G$1" pin="P1" pad="10"/>
<connect gate="G$1" pin="P10" pad="16"/>
<connect gate="G$1" pin="P11" pad="17"/>
<connect gate="G$1" pin="P12" pad="18"/>
<connect gate="G$1" pin="P13" pad="19"/>
<connect gate="G$1" pin="P14" pad="20"/>
<connect gate="G$1" pin="P15" pad="21"/>
<connect gate="G$1" pin="P16" pad="22"/>
<connect gate="G$1" pin="P2" pad="9"/>
<connect gate="G$1" pin="P3" pad="8"/>
<connect gate="G$1" pin="P4" pad="7"/>
<connect gate="G$1" pin="P5" pad="6"/>
<connect gate="G$1" pin="P6" pad="5"/>
<connect gate="G$1" pin="P7" pad="4"/>
<connect gate="G$1" pin="P8" pad="3"/>
<connect gate="G$1" pin="P9" pad="15"/>
<connect gate="G$1" pin="SCL" pad="24"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VEE" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SAA1064/N2,112"/>
<attribute name="OC_FARNELL" value="1627002"/>
<attribute name="OC_NEWARK" value="70R8646"/>
</technology>
</technologies>
</device>
<device name="T" package="SO24">
<connects>
<connect gate="G$1" pin="ADR" pad="1"/>
<connect gate="G$1" pin="CEXT" pad="2"/>
<connect gate="G$1" pin="MX1" pad="11"/>
<connect gate="G$1" pin="MX2" pad="14"/>
<connect gate="G$1" pin="P1" pad="10"/>
<connect gate="G$1" pin="P10" pad="16"/>
<connect gate="G$1" pin="P11" pad="17"/>
<connect gate="G$1" pin="P12" pad="18"/>
<connect gate="G$1" pin="P13" pad="19"/>
<connect gate="G$1" pin="P14" pad="20"/>
<connect gate="G$1" pin="P15" pad="21"/>
<connect gate="G$1" pin="P16" pad="22"/>
<connect gate="G$1" pin="P2" pad="9"/>
<connect gate="G$1" pin="P3" pad="8"/>
<connect gate="G$1" pin="P4" pad="7"/>
<connect gate="G$1" pin="P5" pad="6"/>
<connect gate="G$1" pin="P6" pad="5"/>
<connect gate="G$1" pin="P7" pad="4"/>
<connect gate="G$1" pin="P8" pad="3"/>
<connect gate="G$1" pin="P9" pad="15"/>
<connect gate="G$1" pin="SCL" pad="24"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VEE" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SAA1064T/N2,118"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R8648"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8574" prefix="IC">
<description>I2C-Bus &lt;b&gt;Remote 8-bit I/O expander&lt;/b&gt;&lt;p&gt;
http://www.semiconductors.philips.com/acrobat_download/datasheets/PCF8574_4.pdf</description>
<gates>
<gate name="G$1" symbol="PCF8574"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!INT" pad="13"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="P0" pad="4"/>
<connect gate="G$1" pin="P1" pad="5"/>
<connect gate="G$1" pin="P2" pad="6"/>
<connect gate="G$1" pin="P3" pad="7"/>
<connect gate="G$1" pin="P4" pad="9"/>
<connect gate="G$1" pin="P5" pad="10"/>
<connect gate="G$1" pin="P6" pad="11"/>
<connect gate="G$1" pin="P7" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCF8574PN"/>
<attribute name="OC_FARNELL" value="204020"/>
<attribute name="OC_NEWARK" value="11N8515"/>
</technology>
</technologies>
</device>
<device name="T" package="SO16W">
<connects>
<connect gate="G$1" pin="!INT" pad="13"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="P0" pad="4"/>
<connect gate="G$1" pin="P1" pad="5"/>
<connect gate="G$1" pin="P2" pad="6"/>
<connect gate="G$1" pin="P3" pad="7"/>
<connect gate="G$1" pin="P4" pad="9"/>
<connect gate="G$1" pin="P5" pad="10"/>
<connect gate="G$1" pin="P6" pad="11"/>
<connect gate="G$1" pin="P7" pad="12"/>
<connect gate="G$1" pin="SCL" pad="14"/>
<connect gate="G$1" pin="SDA" pad="15"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCF8574T/3,512"/>
<attribute name="OC_FARNELL" value="1201255"/>
<attribute name="OC_NEWARK" value="70R6870"/>
</technology>
</technologies>
</device>
<device name="TS" package="SSOP20">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="A1" pad="7"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="P0" pad="10"/>
<connect gate="G$1" pin="P1" pad="11"/>
<connect gate="G$1" pin="P2" pad="12"/>
<connect gate="G$1" pin="P3" pad="14"/>
<connect gate="G$1" pin="P4" pad="16"/>
<connect gate="G$1" pin="P5" pad="17"/>
<connect gate="G$1" pin="P6" pad="19"/>
<connect gate="G$1" pin="P7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="VDD" pad="5"/>
<connect gate="G$1" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCF8574TS/3,118"/>
<attribute name="OC_FARNELL" value="1506644"/>
<attribute name="OC_NEWARK" value="70R6873"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8591" prefix="IC">
<description>I2C-Bus &lt;b&gt;D/A CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8591"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AIN0" pad="1"/>
<connect gate="G$1" pin="AIN1" pad="2"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3" pad="4"/>
<connect gate="G$1" pin="AOUT" pad="15"/>
<connect gate="G$1" pin="EXT" pad="12"/>
<connect gate="G$1" pin="OSC" pad="11"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="14"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="PCF8591P"/>
<attribute name="OC_FARNELL" value="396412"/>
<attribute name="OC_NEWARK" value="07WX3385"/>
</technology>
</technologies>
</device>
<device name="T" package="SO16W">
<connects>
<connect gate="G$1" pin="A0" pad="5"/>
<connect gate="G$1" pin="A1" pad="6"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="AGND" pad="13"/>
<connect gate="G$1" pin="AIN0" pad="1"/>
<connect gate="G$1" pin="AIN1" pad="2"/>
<connect gate="G$1" pin="AIN2" pad="3"/>
<connect gate="G$1" pin="AIN3" pad="4"/>
<connect gate="G$1" pin="AOUT" pad="15"/>
<connect gate="G$1" pin="EXT" pad="12"/>
<connect gate="G$1" pin="OSC" pad="11"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="9"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VREF" pad="14"/>
<connect gate="G$1" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCF8591T/2,512"/>
<attribute name="OC_FARNELL" value="1826767"/>
<attribute name="OC_NEWARK" value="70R6911"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8573" prefix="IC">
<description>I2C-Bus &lt;b&gt;CLOCK/CALENDAR&lt;/b&gt;&lt;p&gt;
with power fail detector</description>
<gates>
<gate name="G$1" symbol="PCF8573"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="EXTPF" pad="6"/>
<connect gate="G$1" pin="FSET" pad="11"/>
<connect gate="G$1" pin="MIN" pad="9"/>
<connect gate="G$1" pin="OSCI" pad="13"/>
<connect gate="G$1" pin="OSCO" pad="14"/>
<connect gate="G$1" pin="PFIN" pad="7"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SEC" pad="10"/>
<connect gate="G$1" pin="TEST" pad="12"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS@1" pad="15"/>
<connect gate="G$1" pin="VSS@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="T" package="SO16W">
<connects>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="EXTPF" pad="6"/>
<connect gate="G$1" pin="FSET" pad="11"/>
<connect gate="G$1" pin="MIN" pad="9"/>
<connect gate="G$1" pin="OSCI" pad="13"/>
<connect gate="G$1" pin="OSCO" pad="14"/>
<connect gate="G$1" pin="PFIN" pad="7"/>
<connect gate="G$1" pin="SCL" pad="5"/>
<connect gate="G$1" pin="SDA" pad="4"/>
<connect gate="G$1" pin="SEC" pad="10"/>
<connect gate="G$1" pin="TEST" pad="12"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS@1" pad="15"/>
<connect gate="G$1" pin="VSS@2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P82C150" prefix="IC">
<description>CAN BUS &lt;b&gt;I/O DEVICE&lt;/b&gt;, SLIO&lt;p&gt;
with digital and analog port functions</description>
<gates>
<gate name="G$1" symbol="P82C150"/>
</gates>
<devices>
<device name="" package="SO28">
<connects>
<connect gate="G$1" pin="AVDD" pad="18"/>
<connect gate="G$1" pin="AVSS" pad="20"/>
<connect gate="G$1" pin="CLK/P0" pad="27"/>
<connect gate="G$1" pin="P1" pad="28"/>
<connect gate="G$1" pin="P10" pad="11"/>
<connect gate="G$1" pin="P11" pad="12"/>
<connect gate="G$1" pin="P12" pad="13"/>
<connect gate="G$1" pin="P13" pad="14"/>
<connect gate="G$1" pin="P14" pad="15"/>
<connect gate="G$1" pin="P15" pad="16"/>
<connect gate="G$1" pin="P16" pad="17"/>
<connect gate="G$1" pin="P2" pad="1"/>
<connect gate="G$1" pin="P3" pad="2"/>
<connect gate="G$1" pin="P4" pad="3"/>
<connect gate="G$1" pin="P5" pad="5"/>
<connect gate="G$1" pin="P6" pad="6"/>
<connect gate="G$1" pin="P7" pad="7"/>
<connect gate="G$1" pin="P8" pad="9"/>
<connect gate="G$1" pin="P9" pad="10"/>
<connect gate="G$1" pin="REF" pad="19"/>
<connect gate="G$1" pin="RESET" pad="23"/>
<connect gate="G$1" pin="RX0" pad="21"/>
<connect gate="G$1" pin="RX1" pad="22"/>
<connect gate="G$1" pin="TX0" pad="25"/>
<connect gate="G$1" pin="TX1" pad="26"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
<connect gate="G$1" pin="XMOD" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA82C250" prefix="IC">
<description>&lt;b&gt;CAN CONTROLLER INTERFACE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="P82C250"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="3692358"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="T" package="SO8">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="RS" pad="8"/>
<connect gate="G$1" pin="RXD" pad="4"/>
<connect gate="G$1" pin="TXD" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1085275"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UDA1320ATS" prefix="IC">
<description>Stereo filter &lt;b&gt;D/A CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UDA1320"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="G$1" pin="APPL0" pad="11"/>
<connect gate="G$1" pin="APPL1" pad="10"/>
<connect gate="G$1" pin="APPL2" pad="9"/>
<connect gate="G$1" pin="APPL3" pad="8"/>
<connect gate="G$1" pin="APPSEL" pad="7"/>
<connect gate="G$1" pin="BCK" pad="1"/>
<connect gate="G$1" pin="DATAI" pad="3"/>
<connect gate="G$1" pin="SYSCLK" pad="6"/>
<connect gate="G$1" pin="VDDA" pad="13"/>
<connect gate="G$1" pin="VDDD" pad="4"/>
<connect gate="G$1" pin="VOUTL" pad="14"/>
<connect gate="G$1" pin="VOUTR" pad="16"/>
<connect gate="G$1" pin="VREFDAC" pad="12"/>
<connect gate="G$1" pin="VSSA" pad="15"/>
<connect gate="G$1" pin="VSSD" pad="5"/>
<connect gate="G$1" pin="WS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UDA1360TS" prefix="IC">
<description>Stereo audio &lt;b&gt;A/D CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UDA1360T"/>
</gates>
<devices>
<device name="" package="SSOP16">
<connects>
<connect gate="G$1" pin="BCK" pad="11"/>
<connect gate="G$1" pin="DATAO" pad="13"/>
<connect gate="G$1" pin="FSEL" pad="14"/>
<connect gate="G$1" pin="PWON" pad="7"/>
<connect gate="G$1" pin="SFOR" pad="6"/>
<connect gate="G$1" pin="SYSCLK" pad="8"/>
<connect gate="G$1" pin="VDDA" pad="16"/>
<connect gate="G$1" pin="VDDD" pad="9"/>
<connect gate="G$1" pin="VINL" pad="1"/>
<connect gate="G$1" pin="VINR" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
<connect gate="G$1" pin="VREFN" pad="4"/>
<connect gate="G$1" pin="VREFP" pad="5"/>
<connect gate="G$1" pin="VSSA" pad="15"/>
<connect gate="G$1" pin="VSSD" pad="10"/>
<connect gate="G$1" pin="WS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PFC8583" prefix="IC">
<description>I2C-Bus &lt;b&gt;CLOCK/CALENDAR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PFC8583"/>
</gates>
<devices>
<device name="T" package="SO8-7_5">
<connects>
<connect gate="G$1" pin="!INT" pad="7"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="!INT" pad="7"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="OSCI" pad="1"/>
<connect gate="G$1" pin="OSCO" pad="2"/>
<connect gate="G$1" pin="SCL" pad="6"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="VDD" pad="8"/>
<connect gate="G$1" pin="VSS" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCF8584" prefix="IC">
<description>I2C-Bus &lt;b&gt;CONTROLLER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCF8584"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="!CS" pad="17"/>
<connect gate="G$1" pin="!IACK" pad="4"/>
<connect gate="G$1" pin="!INT" pad="5"/>
<connect gate="G$1" pin="!RD" pad="16"/>
<connect gate="G$1" pin="!RESET" pad="19"/>
<connect gate="G$1" pin="!WR" pad="18"/>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="11"/>
<connect gate="G$1" pin="DB4" pad="12"/>
<connect gate="G$1" pin="DB5" pad="13"/>
<connect gate="G$1" pin="DB6" pad="14"/>
<connect gate="G$1" pin="DB7" pad="15"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="PCF8584P,112"/>
<attribute name="OC_FARNELL" value="8906220"/>
<attribute name="OC_NEWARK" value="18K6671"/>
</technology>
</technologies>
</device>
<device name="T" package="SO20W">
<connects>
<connect gate="G$1" pin="!CS" pad="17"/>
<connect gate="G$1" pin="!IACK" pad="4"/>
<connect gate="G$1" pin="!INT" pad="5"/>
<connect gate="G$1" pin="!RD" pad="16"/>
<connect gate="G$1" pin="!RESET" pad="19"/>
<connect gate="G$1" pin="!WR" pad="18"/>
<connect gate="G$1" pin="A0" pad="6"/>
<connect gate="G$1" pin="CLK" pad="1"/>
<connect gate="G$1" pin="DB0" pad="7"/>
<connect gate="G$1" pin="DB1" pad="8"/>
<connect gate="G$1" pin="DB2" pad="9"/>
<connect gate="G$1" pin="DB3" pad="11"/>
<connect gate="G$1" pin="DB4" pad="12"/>
<connect gate="G$1" pin="DB5" pad="13"/>
<connect gate="G$1" pin="DB6" pad="14"/>
<connect gate="G$1" pin="DB7" pad="15"/>
<connect gate="G$1" pin="SCL" pad="3"/>
<connect gate="G$1" pin="SDA" pad="2"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VSS" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCF8584T/2,512"/>
<attribute name="OC_FARNELL" value="1831225"/>
<attribute name="OC_NEWARK" value="70R6908"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UAA3220TS" prefix="IC">
<description>&lt;b&gt;FSK / ASK  Receiver&lt;/b&gt; Frequency Shift Keying / Amplitude Shift Keying</description>
<gates>
<gate name="G$1" symbol="UAA3220TS"/>
</gates>
<devices>
<device name="" package="SSOP24">
<connects>
<connect gate="G$1" pin="CGND" pad="13"/>
<connect gate="G$1" pin="CPA" pad="15"/>
<connect gate="G$1" pin="CPB" pad="16"/>
<connect gate="G$1" pin="CPC" pad="17"/>
<connect gate="G$1" pin="DATA" pad="14"/>
<connect gate="G$1" pin="DEMO1" pad="10"/>
<connect gate="G$1" pin="DEMO2" pad="11"/>
<connect gate="G$1" pin="FA" pad="22"/>
<connect gate="G$1" pin="GND" pad="12"/>
<connect gate="G$1" pin="LFB" pad="19"/>
<connect gate="G$1" pin="LIN" pad="20"/>
<connect gate="G$1" pin="MGND" pad="24"/>
<connect gate="G$1" pin="MIXIN" pad="23"/>
<connect gate="G$1" pin="OGND" pad="1"/>
<connect gate="G$1" pin="OSB" pad="3"/>
<connect gate="G$1" pin="OSC" pad="5"/>
<connect gate="G$1" pin="OSE" pad="2"/>
<connect gate="G$1" pin="PWD" pad="9"/>
<connect gate="G$1" pin="RSSI" pad="18"/>
<connect gate="G$1" pin="TEM" pad="6"/>
<connect gate="G$1" pin="TN" pad="7"/>
<connect gate="G$1" pin="TP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VCCI" pad="21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="UAA3220TS/V1,118"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R9521"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8*C652-QFP44" prefix="IC">
<description>&lt;b&gt;CMOS single-chip 8-bit Microcontroller&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C52"/>
</gates>
<devices>
<device name="" package="QFP44_SOT307-2">
<connects>
<connect gate="G$1" pin="!EA" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="NC" pad="17"/>
<connect gate="G$1" pin="P00" pad="37"/>
<connect gate="G$1" pin="P01" pad="36"/>
<connect gate="G$1" pin="P02" pad="35"/>
<connect gate="G$1" pin="P03" pad="34"/>
<connect gate="G$1" pin="P04" pad="33"/>
<connect gate="G$1" pin="P05" pad="32"/>
<connect gate="G$1" pin="P06" pad="31"/>
<connect gate="G$1" pin="P07" pad="30"/>
<connect gate="G$1" pin="P10" pad="40"/>
<connect gate="G$1" pin="P11" pad="41"/>
<connect gate="G$1" pin="P12" pad="42"/>
<connect gate="G$1" pin="P13" pad="43"/>
<connect gate="G$1" pin="P14" pad="44"/>
<connect gate="G$1" pin="P15" pad="1"/>
<connect gate="G$1" pin="P16" pad="2"/>
<connect gate="G$1" pin="P17" pad="3"/>
<connect gate="G$1" pin="P20" pad="18"/>
<connect gate="G$1" pin="P21" pad="19"/>
<connect gate="G$1" pin="P22" pad="20"/>
<connect gate="G$1" pin="P23" pad="21"/>
<connect gate="G$1" pin="P24" pad="22"/>
<connect gate="G$1" pin="P25" pad="23"/>
<connect gate="G$1" pin="P26" pad="24"/>
<connect gate="G$1" pin="P27" pad="25"/>
<connect gate="G$1" pin="P30" pad="5"/>
<connect gate="G$1" pin="P31" pad="7"/>
<connect gate="G$1" pin="P32" pad="8"/>
<connect gate="G$1" pin="P33" pad="9"/>
<connect gate="G$1" pin="P34" pad="10"/>
<connect gate="G$1" pin="P35" pad="11"/>
<connect gate="G$1" pin="P36" pad="12"/>
<connect gate="G$1" pin="P37" pad="13"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VDD" pad="38"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="VSS@1" pad="39"/>
<connect gate="G$1" pin="VSS@2" pad="28"/>
<connect gate="G$1" pin="VSS@3" pad="6"/>
<connect gate="G$1" pin="X1" pad="15"/>
<connect gate="G$1" pin="X2" pad="14"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8*C652-PLCC44" prefix="IC">
<description>&lt;b&gt;CMOS single-chip 8-bit Microcontroller&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C52-PLCC44"/>
</gates>
<devices>
<device name="" package="PLCC44S">
<connects>
<connect gate="G$1" pin="!EA" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="32"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="23"/>
<connect gate="G$1" pin="NC@3" pad="34"/>
<connect gate="G$1" pin="P00" pad="43"/>
<connect gate="G$1" pin="P01" pad="42"/>
<connect gate="G$1" pin="P02" pad="41"/>
<connect gate="G$1" pin="P03" pad="40"/>
<connect gate="G$1" pin="P04" pad="39"/>
<connect gate="G$1" pin="P05" pad="38"/>
<connect gate="G$1" pin="P06" pad="37"/>
<connect gate="G$1" pin="P07" pad="36"/>
<connect gate="G$1" pin="P10" pad="2"/>
<connect gate="G$1" pin="P11" pad="3"/>
<connect gate="G$1" pin="P12" pad="4"/>
<connect gate="G$1" pin="P13" pad="5"/>
<connect gate="G$1" pin="P14" pad="6"/>
<connect gate="G$1" pin="P15" pad="7"/>
<connect gate="G$1" pin="P16" pad="8"/>
<connect gate="G$1" pin="P17" pad="9"/>
<connect gate="G$1" pin="P20" pad="24"/>
<connect gate="G$1" pin="P21" pad="25"/>
<connect gate="G$1" pin="P22" pad="26"/>
<connect gate="G$1" pin="P23" pad="27"/>
<connect gate="G$1" pin="P24" pad="28"/>
<connect gate="G$1" pin="P25" pad="29"/>
<connect gate="G$1" pin="P26" pad="30"/>
<connect gate="G$1" pin="P27" pad="31"/>
<connect gate="G$1" pin="P30" pad="11"/>
<connect gate="G$1" pin="P31" pad="13"/>
<connect gate="G$1" pin="P32" pad="14"/>
<connect gate="G$1" pin="P33" pad="15"/>
<connect gate="G$1" pin="P34" pad="16"/>
<connect gate="G$1" pin="P35" pad="17"/>
<connect gate="G$1" pin="P36" pad="18"/>
<connect gate="G$1" pin="P37" pad="19"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VDD" pad="44"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="X1" pad="21"/>
<connect gate="G$1" pin="X2" pad="20"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8*" prefix="IC">
<description>&lt;b&gt;CMOS single-chip 8-bit Microcontroller&lt;/b&gt;&lt;p&gt;
80C31/32 pin compatible</description>
<gates>
<gate name="G$1" symbol="80C52DIL40"/>
</gates>
<devices>
<device name="PN" package="DIL40">
<connects>
<connect gate="G$1" pin="!EA" pad="31"/>
<connect gate="G$1" pin="!PSEN" pad="29"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="P00" pad="39"/>
<connect gate="G$1" pin="P01" pad="38"/>
<connect gate="G$1" pin="P02" pad="37"/>
<connect gate="G$1" pin="P03" pad="36"/>
<connect gate="G$1" pin="P04" pad="35"/>
<connect gate="G$1" pin="P05" pad="34"/>
<connect gate="G$1" pin="P06" pad="33"/>
<connect gate="G$1" pin="P07" pad="32"/>
<connect gate="G$1" pin="P10" pad="1"/>
<connect gate="G$1" pin="P11" pad="2"/>
<connect gate="G$1" pin="P12" pad="3"/>
<connect gate="G$1" pin="P13" pad="4"/>
<connect gate="G$1" pin="P14" pad="5"/>
<connect gate="G$1" pin="P15" pad="6"/>
<connect gate="G$1" pin="P16" pad="7"/>
<connect gate="G$1" pin="P17" pad="8"/>
<connect gate="G$1" pin="P20" pad="21"/>
<connect gate="G$1" pin="P21" pad="22"/>
<connect gate="G$1" pin="P22" pad="23"/>
<connect gate="G$1" pin="P23" pad="24"/>
<connect gate="G$1" pin="P24" pad="25"/>
<connect gate="G$1" pin="P25" pad="26"/>
<connect gate="G$1" pin="P26" pad="27"/>
<connect gate="G$1" pin="P27" pad="28"/>
<connect gate="G$1" pin="P30" pad="10"/>
<connect gate="G$1" pin="P31" pad="11"/>
<connect gate="G$1" pin="P32" pad="12"/>
<connect gate="G$1" pin="P33" pad="13"/>
<connect gate="G$1" pin="P34" pad="14"/>
<connect gate="G$1" pin="P35" pad="15"/>
<connect gate="G$1" pin="P36" pad="16"/>
<connect gate="G$1" pin="P37" pad="17"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="VDD" pad="40"/>
<connect gate="G$1" pin="VSS" pad="20"/>
<connect gate="G$1" pin="X1" pad="19"/>
<connect gate="G$1" pin="X2" pad="18"/>
</connects>
<technologies>
<technology name="0C31SB">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="P80C31SBPN"/>
<attribute name="OC_FARNELL" value="120509"/>
<attribute name="OC_NEWARK" value="67C9971"/>
</technology>
<technology name="0C31SF">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="P80C31SBPN"/>
<attribute name="OC_FARNELL" value="120509"/>
<attribute name="OC_NEWARK" value="67C9971"/>
</technology>
<technology name="0C32SB">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="P80C32SBPN"/>
<attribute name="OC_FARNELL" value="121071"/>
<attribute name="OC_NEWARK" value="67C9973"/>
</technology>
<technology name="0C32SF">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="P80C32SBPN"/>
<attribute name="OC_FARNELL" value="121071"/>
<attribute name="OC_NEWARK" value="67C9973"/>
</technology>
<technology name="0C32UB">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0C32UF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0C652">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3C652">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="AA" package="PLCC44S">
<connects>
<connect gate="G$1" pin="!EA" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="32"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="P00" pad="43"/>
<connect gate="G$1" pin="P01" pad="42"/>
<connect gate="G$1" pin="P02" pad="41"/>
<connect gate="G$1" pin="P03" pad="40"/>
<connect gate="G$1" pin="P04" pad="39"/>
<connect gate="G$1" pin="P05" pad="38"/>
<connect gate="G$1" pin="P06" pad="37"/>
<connect gate="G$1" pin="P07" pad="36"/>
<connect gate="G$1" pin="P10" pad="2"/>
<connect gate="G$1" pin="P11" pad="3"/>
<connect gate="G$1" pin="P12" pad="4"/>
<connect gate="G$1" pin="P13" pad="5"/>
<connect gate="G$1" pin="P14" pad="6"/>
<connect gate="G$1" pin="P15" pad="7"/>
<connect gate="G$1" pin="P16" pad="8"/>
<connect gate="G$1" pin="P17" pad="9"/>
<connect gate="G$1" pin="P20" pad="24"/>
<connect gate="G$1" pin="P21" pad="25"/>
<connect gate="G$1" pin="P22" pad="26"/>
<connect gate="G$1" pin="P23" pad="27"/>
<connect gate="G$1" pin="P24" pad="28"/>
<connect gate="G$1" pin="P25" pad="29"/>
<connect gate="G$1" pin="P26" pad="30"/>
<connect gate="G$1" pin="P27" pad="31"/>
<connect gate="G$1" pin="P30" pad="11"/>
<connect gate="G$1" pin="P31" pad="13"/>
<connect gate="G$1" pin="P32" pad="14"/>
<connect gate="G$1" pin="P33" pad="15"/>
<connect gate="G$1" pin="P34" pad="16"/>
<connect gate="G$1" pin="P35" pad="17"/>
<connect gate="G$1" pin="P36" pad="18"/>
<connect gate="G$1" pin="P37" pad="19"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="VDD" pad="44"/>
<connect gate="G$1" pin="VSS" pad="22"/>
<connect gate="G$1" pin="X1" pad="21"/>
<connect gate="G$1" pin="X2" pad="20"/>
</connects>
<technologies>
<technology name="0C31SB">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C31SBAA,512"/>
<attribute name="OC_FARNELL" value="1831226"/>
<attribute name="OC_NEWARK" value="70R8431"/>
</technology>
<technology name="0C31SF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0C32SB">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C32SBAA,512"/>
<attribute name="OC_FARNELL" value="1831229"/>
<attribute name="OC_NEWARK" value="70R8434"/>
</technology>
<technology name="0C32SF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1831229"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0C32UB">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C32UBAA"/>
<attribute name="OC_FARNELL" value="1201265"/>
<attribute name="OC_NEWARK" value="24M6583"/>
</technology>
<technology name="0C32UF">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C32UFAA,512"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R8437"/>
</technology>
</technologies>
</device>
<device name="BB" package="QFP44_SOT307-2">
<connects>
<connect gate="G$1" pin="!EA" pad="29"/>
<connect gate="G$1" pin="!PSEN" pad="26"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="P00" pad="37"/>
<connect gate="G$1" pin="P01" pad="36"/>
<connect gate="G$1" pin="P02" pad="35"/>
<connect gate="G$1" pin="P03" pad="34"/>
<connect gate="G$1" pin="P04" pad="33"/>
<connect gate="G$1" pin="P05" pad="32"/>
<connect gate="G$1" pin="P06" pad="31"/>
<connect gate="G$1" pin="P07" pad="30"/>
<connect gate="G$1" pin="P10" pad="40"/>
<connect gate="G$1" pin="P11" pad="41"/>
<connect gate="G$1" pin="P12" pad="42"/>
<connect gate="G$1" pin="P13" pad="43"/>
<connect gate="G$1" pin="P14" pad="44"/>
<connect gate="G$1" pin="P15" pad="1"/>
<connect gate="G$1" pin="P16" pad="2"/>
<connect gate="G$1" pin="P17" pad="3"/>
<connect gate="G$1" pin="P20" pad="18"/>
<connect gate="G$1" pin="P21" pad="19"/>
<connect gate="G$1" pin="P22" pad="20"/>
<connect gate="G$1" pin="P23" pad="21"/>
<connect gate="G$1" pin="P24" pad="22"/>
<connect gate="G$1" pin="P25" pad="23"/>
<connect gate="G$1" pin="P26" pad="24"/>
<connect gate="G$1" pin="P27" pad="25"/>
<connect gate="G$1" pin="P30" pad="5"/>
<connect gate="G$1" pin="P31" pad="7"/>
<connect gate="G$1" pin="P32" pad="8"/>
<connect gate="G$1" pin="P33" pad="9"/>
<connect gate="G$1" pin="P34" pad="10"/>
<connect gate="G$1" pin="P35" pad="11"/>
<connect gate="G$1" pin="P36" pad="12"/>
<connect gate="G$1" pin="P37" pad="13"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="VDD" pad="38"/>
<connect gate="G$1" pin="VSS" pad="16"/>
<connect gate="G$1" pin="X1" pad="15"/>
<connect gate="G$1" pin="X2" pad="14"/>
</connects>
<technologies>
<technology name="0C31SB">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C31SBBB,557"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R8432"/>
</technology>
<technology name="0C31SF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0C32SB">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0C32SF">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0C32UB">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0C32UF">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C32UFBB,557"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R8438"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C592" prefix="IC">
<description>&lt;b&gt;8051 -compatible 8bit Microcontroller CAN 2.0A&lt;/b&gt;</description>
<gates>
<gate name="G" symbol="8XC592"/>
<gate name="P" symbol="PWR"/>
</gates>
<devices>
<device name="SOCKEL" package="PLCC-S68">
<connects>
<connect gate="G" pin="/EW" pad="6"/>
<connect gate="G" pin="ALE" pad="45"/>
<connect gate="G" pin="CRX0" pad="57"/>
<connect gate="G" pin="CRX1" pad="56"/>
<connect gate="G" pin="CTX0" pad="23"/>
<connect gate="G" pin="CTX1" pad="24"/>
<connect gate="G" pin="EA" pad="46"/>
<connect gate="G" pin="INT2" pad="16"/>
<connect gate="G" pin="INT3" pad="17"/>
<connect gate="G" pin="INT4" pad="18"/>
<connect gate="G" pin="INT5" pad="19"/>
<connect gate="G" pin="P0.0/D0" pad="54"/>
<connect gate="G" pin="P0.1/D1" pad="53"/>
<connect gate="G" pin="P0.2/D2" pad="52"/>
<connect gate="G" pin="P0.3/D3" pad="51"/>
<connect gate="G" pin="P0.4/D4" pad="50"/>
<connect gate="G" pin="P0.5/D5" pad="49"/>
<connect gate="G" pin="P0.6/D6" pad="48"/>
<connect gate="G" pin="P0.7/D7" pad="47"/>
<connect gate="G" pin="P2.0/A8" pad="36"/>
<connect gate="G" pin="P2.1/A9" pad="37"/>
<connect gate="G" pin="P2.2/A10" pad="38"/>
<connect gate="G" pin="P2.3/A11" pad="39"/>
<connect gate="G" pin="P2.4/A12" pad="40"/>
<connect gate="G" pin="P2.5/A13" pad="41"/>
<connect gate="G" pin="P2.6/A14" pad="42"/>
<connect gate="G" pin="P2.7/A15" pad="43"/>
<connect gate="G" pin="P3.0" pad="25"/>
<connect gate="G" pin="P3.1" pad="26"/>
<connect gate="G" pin="P3.2" pad="27"/>
<connect gate="G" pin="P3.3" pad="28"/>
<connect gate="G" pin="P3.4/T0" pad="29"/>
<connect gate="G" pin="P3.5/T1" pad="30"/>
<connect gate="G" pin="P3.6/WR" pad="31"/>
<connect gate="G" pin="P3.7/RD" pad="32"/>
<connect gate="G" pin="P4.0" pad="7"/>
<connect gate="G" pin="P4.1" pad="8"/>
<connect gate="G" pin="P4.2" pad="9"/>
<connect gate="G" pin="P4.3" pad="10"/>
<connect gate="G" pin="P4.4" pad="11"/>
<connect gate="G" pin="P4.5" pad="12"/>
<connect gate="G" pin="P4.6" pad="13"/>
<connect gate="G" pin="P4.7" pad="14"/>
<connect gate="G" pin="P5.0/AN0" pad="1"/>
<connect gate="G" pin="P5.1/AN1" pad="68"/>
<connect gate="G" pin="P5.2/AN2" pad="67"/>
<connect gate="G" pin="P5.3/AN3" pad="66"/>
<connect gate="G" pin="P5.4/AN4" pad="65"/>
<connect gate="G" pin="P5.5/AN5" pad="64"/>
<connect gate="G" pin="P5.6/AN6" pad="63"/>
<connect gate="G" pin="P5.7/AN7" pad="62"/>
<connect gate="G" pin="PSEN" pad="44"/>
<connect gate="G" pin="PWM0" pad="4"/>
<connect gate="G" pin="PWM1" pad="5"/>
<connect gate="G" pin="REF" pad="55"/>
<connect gate="G" pin="RST" pad="15"/>
<connect gate="G" pin="RT2" pad="21"/>
<connect gate="G" pin="STADC" pad="3"/>
<connect gate="G" pin="T2" pad="20"/>
<connect gate="G" pin="VAGND" pad="58"/>
<connect gate="G" pin="VAREF" pad="59"/>
<connect gate="G" pin="XTAL1" pad="34"/>
<connect gate="G" pin="XTAL2" pad="33"/>
<connect gate="P" pin="AGND" pad="60"/>
<connect gate="P" pin="AVCC" pad="61"/>
<connect gate="P" pin="CGND" pad="22"/>
<connect gate="P" pin="GND" pad="35"/>
<connect gate="P" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SMD" package="PLCC68">
<connects>
<connect gate="G" pin="/EW" pad="6"/>
<connect gate="G" pin="ALE" pad="45"/>
<connect gate="G" pin="CRX0" pad="57"/>
<connect gate="G" pin="CRX1" pad="56"/>
<connect gate="G" pin="CTX0" pad="23"/>
<connect gate="G" pin="CTX1" pad="24"/>
<connect gate="G" pin="EA" pad="46"/>
<connect gate="G" pin="INT2" pad="16"/>
<connect gate="G" pin="INT3" pad="17"/>
<connect gate="G" pin="INT4" pad="18"/>
<connect gate="G" pin="INT5" pad="19"/>
<connect gate="G" pin="P0.0/D0" pad="54"/>
<connect gate="G" pin="P0.1/D1" pad="53"/>
<connect gate="G" pin="P0.2/D2" pad="52"/>
<connect gate="G" pin="P0.3/D3" pad="51"/>
<connect gate="G" pin="P0.4/D4" pad="50"/>
<connect gate="G" pin="P0.5/D5" pad="49"/>
<connect gate="G" pin="P0.6/D6" pad="48"/>
<connect gate="G" pin="P0.7/D7" pad="47"/>
<connect gate="G" pin="P2.0/A8" pad="36"/>
<connect gate="G" pin="P2.1/A9" pad="37"/>
<connect gate="G" pin="P2.2/A10" pad="38"/>
<connect gate="G" pin="P2.3/A11" pad="39"/>
<connect gate="G" pin="P2.4/A12" pad="40"/>
<connect gate="G" pin="P2.5/A13" pad="41"/>
<connect gate="G" pin="P2.6/A14" pad="42"/>
<connect gate="G" pin="P2.7/A15" pad="43"/>
<connect gate="G" pin="P3.0" pad="25"/>
<connect gate="G" pin="P3.1" pad="26"/>
<connect gate="G" pin="P3.2" pad="27"/>
<connect gate="G" pin="P3.3" pad="28"/>
<connect gate="G" pin="P3.4/T0" pad="29"/>
<connect gate="G" pin="P3.5/T1" pad="30"/>
<connect gate="G" pin="P3.6/WR" pad="31"/>
<connect gate="G" pin="P3.7/RD" pad="32"/>
<connect gate="G" pin="P4.0" pad="7"/>
<connect gate="G" pin="P4.1" pad="8"/>
<connect gate="G" pin="P4.2" pad="9"/>
<connect gate="G" pin="P4.3" pad="10"/>
<connect gate="G" pin="P4.4" pad="11"/>
<connect gate="G" pin="P4.5" pad="12"/>
<connect gate="G" pin="P4.6" pad="13"/>
<connect gate="G" pin="P4.7" pad="14"/>
<connect gate="G" pin="P5.0/AN0" pad="1"/>
<connect gate="G" pin="P5.1/AN1" pad="68"/>
<connect gate="G" pin="P5.2/AN2" pad="67"/>
<connect gate="G" pin="P5.3/AN3" pad="66"/>
<connect gate="G" pin="P5.4/AN4" pad="65"/>
<connect gate="G" pin="P5.5/AN5" pad="64"/>
<connect gate="G" pin="P5.6/AN6" pad="63"/>
<connect gate="G" pin="P5.7/AN7" pad="62"/>
<connect gate="G" pin="PSEN" pad="44"/>
<connect gate="G" pin="PWM0" pad="4"/>
<connect gate="G" pin="PWM1" pad="5"/>
<connect gate="G" pin="REF" pad="55"/>
<connect gate="G" pin="RST" pad="15"/>
<connect gate="G" pin="RT2" pad="21"/>
<connect gate="G" pin="STADC" pad="3"/>
<connect gate="G" pin="T2" pad="20"/>
<connect gate="G" pin="VAGND" pad="58"/>
<connect gate="G" pin="VAREF" pad="59"/>
<connect gate="G" pin="XTAL1" pad="34"/>
<connect gate="G" pin="XTAL2" pad="33"/>
<connect gate="P" pin="AGND" pad="60"/>
<connect gate="P" pin="AVCC" pad="61"/>
<connect gate="P" pin="CGND" pad="22"/>
<connect gate="P" pin="GND" pad="35"/>
<connect gate="P" pin="VCC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C592FFA/00,512"/>
<attribute name="OC_FARNELL" value="1085276"/>
<attribute name="OC_NEWARK" value="70R8453"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C562" prefix="IC">
<description>&lt;b&gt;8051-compatible 8bit Microcontroller&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="PWR5+2"/>
<gate name="G" symbol="8XC562"/>
</gates>
<devices>
<device name="" package="PLCC-S68">
<connects>
<connect gate="G" pin="/EW" pad="6"/>
<connect gate="G" pin="ALE" pad="48"/>
<connect gate="G" pin="EA" pad="49"/>
<connect gate="G" pin="NC@0" pad="32"/>
<connect gate="G" pin="NC@1" pad="33"/>
<connect gate="G" pin="NC@2" pad="38"/>
<connect gate="G" pin="P0.0/D0" pad="57"/>
<connect gate="G" pin="P0.1/D1" pad="56"/>
<connect gate="G" pin="P0.2/D2" pad="55"/>
<connect gate="G" pin="P0.3/D3" pad="54"/>
<connect gate="G" pin="P0.4/D4" pad="53"/>
<connect gate="G" pin="P0.5/D5" pad="52"/>
<connect gate="G" pin="P0.6/D6" pad="51"/>
<connect gate="G" pin="P0.7/D7" pad="50"/>
<connect gate="G" pin="P1.0/CT0I" pad="16"/>
<connect gate="G" pin="P1.1/CT1I" pad="17"/>
<connect gate="G" pin="P1.2/CT2I" pad="18"/>
<connect gate="G" pin="P1.3/CT3I" pad="19"/>
<connect gate="G" pin="P1.4/T2" pad="20"/>
<connect gate="G" pin="P1.5/RT2" pad="21"/>
<connect gate="G" pin="P1.6" pad="22"/>
<connect gate="G" pin="P1.7" pad="23"/>
<connect gate="G" pin="P2.0/A8" pad="39"/>
<connect gate="G" pin="P2.1/A9" pad="40"/>
<connect gate="G" pin="P2.2/A10" pad="41"/>
<connect gate="G" pin="P2.3/A11" pad="42"/>
<connect gate="G" pin="P2.4/A12" pad="43"/>
<connect gate="G" pin="P2.5/A13" pad="44"/>
<connect gate="G" pin="P2.6/A14" pad="45"/>
<connect gate="G" pin="P2.7/A15" pad="46"/>
<connect gate="G" pin="P3.0" pad="24"/>
<connect gate="G" pin="P3.1" pad="25"/>
<connect gate="G" pin="P3.2" pad="26"/>
<connect gate="G" pin="P3.3" pad="27"/>
<connect gate="G" pin="P3.4/T0" pad="28"/>
<connect gate="G" pin="P3.5/T1" pad="29"/>
<connect gate="G" pin="P3.6/WR" pad="30"/>
<connect gate="G" pin="P3.7/RD" pad="31"/>
<connect gate="G" pin="P4.0/CMSR0" pad="7"/>
<connect gate="G" pin="P4.1/CMSR1" pad="8"/>
<connect gate="G" pin="P4.2/CMSR2" pad="9"/>
<connect gate="G" pin="P4.3/CMSR3" pad="10"/>
<connect gate="G" pin="P4.4/CMSR4" pad="11"/>
<connect gate="G" pin="P4.5/CMSR5" pad="12"/>
<connect gate="G" pin="P4.6/CMT0" pad="13"/>
<connect gate="G" pin="P4.7/CMT1" pad="14"/>
<connect gate="G" pin="P5.0/ADC0" pad="1"/>
<connect gate="G" pin="P5.1/ADC1" pad="68"/>
<connect gate="G" pin="P5.2/ADC2" pad="67"/>
<connect gate="G" pin="P5.3/ADC3" pad="66"/>
<connect gate="G" pin="P5.4/ADC4" pad="65"/>
<connect gate="G" pin="P5.5/ADC5" pad="64"/>
<connect gate="G" pin="P5.6/ADC6" pad="63"/>
<connect gate="G" pin="P5.7/ADC7" pad="62"/>
<connect gate="G" pin="PSEN" pad="47"/>
<connect gate="G" pin="PWM0" pad="4"/>
<connect gate="G" pin="PWM1" pad="5"/>
<connect gate="G" pin="RST" pad="15"/>
<connect gate="G" pin="STADC" pad="3"/>
<connect gate="G" pin="XTAL1" pad="35"/>
<connect gate="G" pin="XTAL2" pad="34"/>
<connect gate="P" pin="AVDD" pad="61"/>
<connect gate="P" pin="AVREF-" pad="58"/>
<connect gate="P" pin="AVSS" pad="60"/>
<connect gate="P" pin="VDD" pad="2"/>
<connect gate="P" pin="VREF" pad="59"/>
<connect gate="P" pin="VSS@0" pad="36"/>
<connect gate="P" pin="VSS@1" pad="37"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P80C562EBA/02,512"/>
<attribute name="OC_FARNELL" value="121198"/>
<attribute name="OC_NEWARK" value="70R8452"/>
</technology>
</technologies>
</device>
<device name="SMD" package="PLCC68">
<connects>
<connect gate="G" pin="/EW" pad="6"/>
<connect gate="G" pin="ALE" pad="48"/>
<connect gate="G" pin="EA" pad="49"/>
<connect gate="G" pin="NC@0" pad="32"/>
<connect gate="G" pin="NC@1" pad="33"/>
<connect gate="G" pin="NC@2" pad="38"/>
<connect gate="G" pin="P0.0/D0" pad="57"/>
<connect gate="G" pin="P0.1/D1" pad="56"/>
<connect gate="G" pin="P0.2/D2" pad="55"/>
<connect gate="G" pin="P0.3/D3" pad="54"/>
<connect gate="G" pin="P0.4/D4" pad="53"/>
<connect gate="G" pin="P0.5/D5" pad="52"/>
<connect gate="G" pin="P0.6/D6" pad="51"/>
<connect gate="G" pin="P0.7/D7" pad="50"/>
<connect gate="G" pin="P1.0/CT0I" pad="16"/>
<connect gate="G" pin="P1.1/CT1I" pad="17"/>
<connect gate="G" pin="P1.2/CT2I" pad="18"/>
<connect gate="G" pin="P1.3/CT3I" pad="19"/>
<connect gate="G" pin="P1.4/T2" pad="20"/>
<connect gate="G" pin="P1.5/RT2" pad="21"/>
<connect gate="G" pin="P1.6" pad="22"/>
<connect gate="G" pin="P1.7" pad="23"/>
<connect gate="G" pin="P2.0/A8" pad="39"/>
<connect gate="G" pin="P2.1/A9" pad="40"/>
<connect gate="G" pin="P2.2/A10" pad="41"/>
<connect gate="G" pin="P2.3/A11" pad="42"/>
<connect gate="G" pin="P2.4/A12" pad="43"/>
<connect gate="G" pin="P2.5/A13" pad="44"/>
<connect gate="G" pin="P2.6/A14" pad="45"/>
<connect gate="G" pin="P2.7/A15" pad="46"/>
<connect gate="G" pin="P3.0" pad="24"/>
<connect gate="G" pin="P3.1" pad="25"/>
<connect gate="G" pin="P3.2" pad="26"/>
<connect gate="G" pin="P3.3" pad="27"/>
<connect gate="G" pin="P3.4/T0" pad="28"/>
<connect gate="G" pin="P3.5/T1" pad="29"/>
<connect gate="G" pin="P3.6/WR" pad="30"/>
<connect gate="G" pin="P3.7/RD" pad="31"/>
<connect gate="G" pin="P4.0/CMSR0" pad="7"/>
<connect gate="G" pin="P4.1/CMSR1" pad="8"/>
<connect gate="G" pin="P4.2/CMSR2" pad="9"/>
<connect gate="G" pin="P4.3/CMSR3" pad="10"/>
<connect gate="G" pin="P4.4/CMSR4" pad="11"/>
<connect gate="G" pin="P4.5/CMSR5" pad="12"/>
<connect gate="G" pin="P4.6/CMT0" pad="13"/>
<connect gate="G" pin="P4.7/CMT1" pad="14"/>
<connect gate="G" pin="P5.0/ADC0" pad="1"/>
<connect gate="G" pin="P5.1/ADC1" pad="68"/>
<connect gate="G" pin="P5.2/ADC2" pad="67"/>
<connect gate="G" pin="P5.3/ADC3" pad="66"/>
<connect gate="G" pin="P5.4/ADC4" pad="65"/>
<connect gate="G" pin="P5.5/ADC5" pad="64"/>
<connect gate="G" pin="P5.6/ADC6" pad="63"/>
<connect gate="G" pin="P5.7/ADC7" pad="62"/>
<connect gate="G" pin="PSEN" pad="47"/>
<connect gate="G" pin="PWM0" pad="4"/>
<connect gate="G" pin="PWM1" pad="5"/>
<connect gate="G" pin="RST" pad="15"/>
<connect gate="G" pin="STADC" pad="3"/>
<connect gate="G" pin="XTAL1" pad="35"/>
<connect gate="G" pin="XTAL2" pad="34"/>
<connect gate="P" pin="AVDD" pad="61"/>
<connect gate="P" pin="AVREF-" pad="58"/>
<connect gate="P" pin="AVSS" pad="60"/>
<connect gate="P" pin="VDD" pad="2"/>
<connect gate="P" pin="VREF" pad="59"/>
<connect gate="P" pin="VSS@0" pad="36"/>
<connect gate="P" pin="VSS@1" pad="37"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="87C751" prefix="IC" uservalue="yes">
<description>&lt;b&gt;83C751/87C751 80C51 with  I2C bus, 8-bit Microcontroller&lt;/b&gt;&lt;p&gt;
2K/64 OTP/ROM</description>
<gates>
<gate name="G" symbol="8XC751"/>
<gate name="P" symbol="PWR2"/>
</gates>
<devices>
<device name="" package="DIP24SKI">
<connects>
<connect gate="G" pin="A0" pad="5"/>
<connect gate="G" pin="A1" pad="4"/>
<connect gate="G" pin="A2" pad="3"/>
<connect gate="G" pin="A3" pad="2"/>
<connect gate="G" pin="A4" pad="1"/>
<connect gate="G" pin="A5" pad="23"/>
<connect gate="G" pin="A6" pad="22"/>
<connect gate="G" pin="A7" pad="21"/>
<connect gate="G" pin="D0" pad="13"/>
<connect gate="G" pin="D1" pad="14"/>
<connect gate="G" pin="D2" pad="15"/>
<connect gate="G" pin="D3" pad="16"/>
<connect gate="G" pin="D4" pad="17"/>
<connect gate="G" pin="D5" pad="18"/>
<connect gate="G" pin="D6" pad="19"/>
<connect gate="G" pin="D7" pad="20"/>
<connect gate="G" pin="RST" pad="9"/>
<connect gate="G" pin="SCL" pad="8"/>
<connect gate="G" pin="SDA" pad="7"/>
<connect gate="G" pin="VPP" pad="6"/>
<connect gate="G" pin="XTAL1" pad="11"/>
<connect gate="G" pin="XTAL2" pad="10"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="87C748" prefix="IC" uservalue="yes">
<description>&lt;b&gt;8051 -comabtible 8bit Microcontroller&lt;/b&gt;</description>
<gates>
<gate name="G" symbol="8XC748"/>
<gate name="P" symbol="PWR2"/>
</gates>
<devices>
<device name="" package="DIP24SKI">
<connects>
<connect gate="G" pin="A0" pad="5"/>
<connect gate="G" pin="A1" pad="4"/>
<connect gate="G" pin="A2" pad="3"/>
<connect gate="G" pin="A3" pad="2"/>
<connect gate="G" pin="A4" pad="1"/>
<connect gate="G" pin="A5" pad="23"/>
<connect gate="G" pin="A6" pad="22"/>
<connect gate="G" pin="A7" pad="21"/>
<connect gate="G" pin="ASEL" pad="8"/>
<connect gate="G" pin="D0" pad="13"/>
<connect gate="G" pin="D1" pad="14"/>
<connect gate="G" pin="D2" pad="15"/>
<connect gate="G" pin="D3" pad="16"/>
<connect gate="G" pin="D4" pad="17"/>
<connect gate="G" pin="D5" pad="18"/>
<connect gate="G" pin="D6" pad="19"/>
<connect gate="G" pin="D7" pad="20"/>
<connect gate="G" pin="OE-PGM" pad="7"/>
<connect gate="G" pin="RESET" pad="9"/>
<connect gate="G" pin="VPP" pad="6"/>
<connect gate="G" pin="X1" pad="11"/>
<connect gate="G" pin="X2" pad="10"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C576" prefix="IC" uservalue="yes">
<description>&lt;b&gt;8051 -compatible 8-bit Microcontroller&lt;p&gt;</description>
<gates>
<gate name="P" symbol="PWR2"/>
<gate name="A" symbol="PWRA"/>
<gate name="G" symbol="8XC576"/>
</gates>
<devices>
<device name="SMD" package="PLCC44">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="AVCC" pad="2"/>
<connect gate="G" pin="ALE" pad="33"/>
<connect gate="G" pin="EA" pad="35"/>
<connect gate="G" pin="NC@0" pad="1"/>
<connect gate="G" pin="NC@1" pad="12"/>
<connect gate="G" pin="NC@2" pad="23"/>
<connect gate="G" pin="NC@3" pad="34"/>
<connect gate="G" pin="P0.0/D0" pad="43"/>
<connect gate="G" pin="P0.1/D1" pad="42"/>
<connect gate="G" pin="P0.2/D2" pad="41"/>
<connect gate="G" pin="P0.3/D3" pad="40"/>
<connect gate="G" pin="P0.4/D4" pad="39"/>
<connect gate="G" pin="P0.5/D5" pad="38"/>
<connect gate="G" pin="P0.6/D6" pad="37"/>
<connect gate="G" pin="P0.7/D7" pad="36"/>
<connect gate="G" pin="P1.0" pad="4"/>
<connect gate="G" pin="P1.1" pad="5"/>
<connect gate="G" pin="P1.2" pad="6"/>
<connect gate="G" pin="P1.3" pad="7"/>
<connect gate="G" pin="P1.4" pad="8"/>
<connect gate="G" pin="P1.5" pad="9"/>
<connect gate="G" pin="P2.0/A8" pad="24"/>
<connect gate="G" pin="P2.1/A9" pad="25"/>
<connect gate="G" pin="P2.2/A10" pad="26"/>
<connect gate="G" pin="P2.3/A11" pad="27"/>
<connect gate="G" pin="P2.4/A12" pad="28"/>
<connect gate="G" pin="P2.5/A13" pad="29"/>
<connect gate="G" pin="P2.6/A14" pad="30"/>
<connect gate="G" pin="P2.7/A15" pad="31"/>
<connect gate="G" pin="P3.0" pad="11"/>
<connect gate="G" pin="P3.1" pad="13"/>
<connect gate="G" pin="P3.2" pad="14"/>
<connect gate="G" pin="P3.3" pad="15"/>
<connect gate="G" pin="P3.4/T0" pad="16"/>
<connect gate="G" pin="P3.5/T1" pad="17"/>
<connect gate="G" pin="P3.6/WR" pad="18"/>
<connect gate="G" pin="P3.7/RD" pad="19"/>
<connect gate="G" pin="PSEN" pad="32"/>
<connect gate="G" pin="RST" pad="10"/>
<connect gate="G" pin="XTAL1" pad="21"/>
<connect gate="G" pin="XTAL2" pad="20"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="VCC" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="PLCC44S">
<connects>
<connect gate="A" pin="AGND" pad="3"/>
<connect gate="A" pin="AVCC" pad="2"/>
<connect gate="G" pin="ALE" pad="33"/>
<connect gate="G" pin="EA" pad="35"/>
<connect gate="G" pin="NC@0" pad="1"/>
<connect gate="G" pin="NC@1" pad="12"/>
<connect gate="G" pin="NC@2" pad="23"/>
<connect gate="G" pin="NC@3" pad="34"/>
<connect gate="G" pin="P0.0/D0" pad="43"/>
<connect gate="G" pin="P0.1/D1" pad="42"/>
<connect gate="G" pin="P0.2/D2" pad="41"/>
<connect gate="G" pin="P0.3/D3" pad="40"/>
<connect gate="G" pin="P0.4/D4" pad="39"/>
<connect gate="G" pin="P0.5/D5" pad="38"/>
<connect gate="G" pin="P0.6/D6" pad="37"/>
<connect gate="G" pin="P0.7/D7" pad="36"/>
<connect gate="G" pin="P1.0" pad="4"/>
<connect gate="G" pin="P1.1" pad="5"/>
<connect gate="G" pin="P1.2" pad="6"/>
<connect gate="G" pin="P1.3" pad="7"/>
<connect gate="G" pin="P1.4" pad="8"/>
<connect gate="G" pin="P1.5" pad="9"/>
<connect gate="G" pin="P2.0/A8" pad="24"/>
<connect gate="G" pin="P2.1/A9" pad="25"/>
<connect gate="G" pin="P2.2/A10" pad="26"/>
<connect gate="G" pin="P2.3/A11" pad="27"/>
<connect gate="G" pin="P2.4/A12" pad="28"/>
<connect gate="G" pin="P2.5/A13" pad="29"/>
<connect gate="G" pin="P2.6/A14" pad="30"/>
<connect gate="G" pin="P2.7/A15" pad="31"/>
<connect gate="G" pin="P3.0" pad="11"/>
<connect gate="G" pin="P3.1" pad="13"/>
<connect gate="G" pin="P3.2" pad="14"/>
<connect gate="G" pin="P3.3" pad="15"/>
<connect gate="G" pin="P3.4/T0" pad="16"/>
<connect gate="G" pin="P3.5/T1" pad="17"/>
<connect gate="G" pin="P3.6/WR" pad="18"/>
<connect gate="G" pin="P3.7/RD" pad="19"/>
<connect gate="G" pin="PSEN" pad="32"/>
<connect gate="G" pin="RST" pad="10"/>
<connect gate="G" pin="XTAL1" pad="21"/>
<connect gate="G" pin="XTAL2" pad="20"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="VCC" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8*CE598" prefix="IC" uservalue="yes">
<description>&lt;b&gt;8bit 8051 Microcontroller, CAN 2.0A&lt;/b&gt;&lt;p&gt;
 Without ROM P80CE598FFB/P80CE598FHB&lt;p&gt;
 With ROM P83CE598FFB/P83CE598FHB</description>
<gates>
<gate name="G" symbol="8XC598"/>
<gate name="P" symbol="PWR5"/>
<gate name="C" symbol="PWRC"/>
<gate name="N" symbol="NC5"/>
</gates>
<devices>
<device name="FP" package="QFP80">
<connects>
<connect gate="C" pin="CGND" pad="37"/>
<connect gate="C" pin="CVCC" pad="40"/>
<connect gate="G" pin="/EW" pad="18"/>
<connect gate="G" pin="ALE" pad="64"/>
<connect gate="G" pin="CRX0" pad="80"/>
<connect gate="G" pin="CRX1" pad="79"/>
<connect gate="G" pin="CTX0" pad="38"/>
<connect gate="G" pin="CTX1" pad="39"/>
<connect gate="G" pin="EA" pad="65"/>
<connect gate="G" pin="INT2" pad="31"/>
<connect gate="G" pin="INT3" pad="32"/>
<connect gate="G" pin="INT4" pad="33"/>
<connect gate="G" pin="INT5" pad="34"/>
<connect gate="G" pin="P0.0/D0" pad="75"/>
<connect gate="G" pin="P0.1/D1" pad="74"/>
<connect gate="G" pin="P0.2/D2" pad="73"/>
<connect gate="G" pin="P0.3/D3" pad="72"/>
<connect gate="G" pin="P0.4/D4" pad="71"/>
<connect gate="G" pin="P0.5/D5" pad="70"/>
<connect gate="G" pin="P0.6/D6" pad="69"/>
<connect gate="G" pin="P0.7/D7" pad="68"/>
<connect gate="G" pin="P2.0/A8" pad="55"/>
<connect gate="G" pin="P2.1/A9" pad="56"/>
<connect gate="G" pin="P2.2/A10" pad="57"/>
<connect gate="G" pin="P2.3/A11" pad="58"/>
<connect gate="G" pin="P2.4/A12" pad="59"/>
<connect gate="G" pin="P2.5/A13" pad="60"/>
<connect gate="G" pin="P2.6/A14" pad="61"/>
<connect gate="G" pin="P2.7/A15" pad="62"/>
<connect gate="G" pin="P3.0" pad="41"/>
<connect gate="G" pin="P3.1" pad="42"/>
<connect gate="G" pin="P3.2" pad="43"/>
<connect gate="G" pin="P3.3" pad="44"/>
<connect gate="G" pin="P3.4/T0" pad="45"/>
<connect gate="G" pin="P3.5/T1" pad="46"/>
<connect gate="G" pin="P3.6/WR" pad="47"/>
<connect gate="G" pin="P3.7/RD" pad="48"/>
<connect gate="G" pin="P4.0" pad="19"/>
<connect gate="G" pin="P4.1" pad="20"/>
<connect gate="G" pin="P4.2" pad="21"/>
<connect gate="G" pin="P4.3" pad="22"/>
<connect gate="G" pin="P4.4" pad="24"/>
<connect gate="G" pin="P4.5" pad="25"/>
<connect gate="G" pin="P4.6" pad="26"/>
<connect gate="G" pin="P4.7" pad="27"/>
<connect gate="G" pin="P5.0/AN0" pad="12"/>
<connect gate="G" pin="P5.1/AN1" pad="11"/>
<connect gate="G" pin="P5.2/AN2" pad="10"/>
<connect gate="G" pin="P5.3/AN3" pad="9"/>
<connect gate="G" pin="P5.4/AN4" pad="8"/>
<connect gate="G" pin="P5.5/AN5" pad="7"/>
<connect gate="G" pin="P5.6/AN6" pad="6"/>
<connect gate="G" pin="P5.7/AN7" pad="5"/>
<connect gate="G" pin="PSEN" pad="63"/>
<connect gate="G" pin="PWM0" pad="16"/>
<connect gate="G" pin="PWM1" pad="17"/>
<connect gate="G" pin="REF" pad="78"/>
<connect gate="G" pin="RST" pad="30"/>
<connect gate="G" pin="RT2" pad="36"/>
<connect gate="G" pin="STADC" pad="15"/>
<connect gate="G" pin="T2" pad="35"/>
<connect gate="G" pin="VAGND" pad="1"/>
<connect gate="G" pin="VAREF" pad="2"/>
<connect gate="G" pin="XTAL1" pad="52"/>
<connect gate="G" pin="XTAL2" pad="51"/>
<connect gate="N" pin="NC@0" pad="23"/>
<connect gate="N" pin="NC@1" pad="49"/>
<connect gate="N" pin="NC@2" pad="50"/>
<connect gate="N" pin="NC@3" pad="66"/>
<connect gate="N" pin="NC@4" pad="67"/>
<connect gate="P" pin="GND@0" pad="13"/>
<connect gate="P" pin="GND@1" pad="29"/>
<connect gate="P" pin="GND@2" pad="54"/>
<connect gate="P" pin="GND@3" pad="77"/>
<connect gate="P" pin="GND@4" pad="3"/>
<connect gate="P" pin="VCC@0" pad="14"/>
<connect gate="P" pin="VCC@1" pad="28"/>
<connect gate="P" pin="VCC@2" pad="53"/>
<connect gate="P" pin="VCC@3" pad="76"/>
<connect gate="P" pin="VCC@4" pad="4"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82B715" prefix="IC" uservalue="yes">
<description>&lt;b&gt;I2C bus extender&lt;/b&gt;</description>
<gates>
<gate name="G" symbol="82B715"/>
<gate name="P" symbol="PWR2"/>
<gate name="NC" symbol="NC2"/>
</gates>
<devices>
<device name="TD" package="SO8">
<connects>
<connect gate="G" pin="LX" pad="2"/>
<connect gate="G" pin="LY" pad="7"/>
<connect gate="G" pin="SX" pad="3"/>
<connect gate="G" pin="SY" pad="6"/>
<connect gate="NC" pin="NC@0" pad="5"/>
<connect gate="NC" pin="NC@1" pad="1"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="P82B715TD,118"/>
<attribute name="OC_FARNELL" value="1627047"/>
<attribute name="OC_NEWARK" value="70R8457"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SJA1000" prefix="IC" uservalue="yes">
<description>&lt;b&gt;BASIC-CAN 2.0a Controller&lt;/b&gt; (former 82C200)&lt;p&gt;
 Stand-alone CAN controller</description>
<gates>
<gate name="G$1" symbol="82C200"/>
<gate name="VDD1" symbol="VDD"/>
<gate name="VDD2" symbol="VDD"/>
<gate name="VDD3" symbol="VDD"/>
<gate name="VSS1" symbol="VSS"/>
<gate name="VSS2" symbol="VSS"/>
<gate name="VSS3" symbol="VSS"/>
</gates>
<devices>
<device name="T" package="SO-28L">
<connects>
<connect gate="G$1" pin="/CS" pad="4"/>
<connect gate="G$1" pin="/INT" pad="16"/>
<connect gate="G$1" pin="/RD" pad="5"/>
<connect gate="G$1" pin="/RST" pad="17"/>
<connect gate="G$1" pin="/WR" pad="6"/>
<connect gate="G$1" pin="AD0" pad="23"/>
<connect gate="G$1" pin="AD1" pad="24"/>
<connect gate="G$1" pin="AD2" pad="25"/>
<connect gate="G$1" pin="AD3" pad="26"/>
<connect gate="G$1" pin="AD4" pad="27"/>
<connect gate="G$1" pin="AD5" pad="28"/>
<connect gate="G$1" pin="AD6" pad="1"/>
<connect gate="G$1" pin="AD7" pad="2"/>
<connect gate="G$1" pin="ALE" pad="3"/>
<connect gate="G$1" pin="CLK_OUT" pad="7"/>
<connect gate="G$1" pin="MODE" pad="11"/>
<connect gate="G$1" pin="RX0" pad="19"/>
<connect gate="G$1" pin="RX1" pad="20"/>
<connect gate="G$1" pin="TX0" pad="13"/>
<connect gate="G$1" pin="TX1" pad="14"/>
<connect gate="G$1" pin="XTAL1" pad="9"/>
<connect gate="G$1" pin="XTAL2" pad="10"/>
<connect gate="VDD1" pin="VDD" pad="22"/>
<connect gate="VDD2" pin="VDD" pad="18"/>
<connect gate="VDD3" pin="VDD" pad="12"/>
<connect gate="VSS1" pin="VSS" pad="8"/>
<connect gate="VSS2" pin="VSS" pad="21"/>
<connect gate="VSS3" pin="VSS" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SJA1000T/N1"/>
<attribute name="OC_FARNELL" value="1775880"/>
<attribute name="OC_NEWARK" value="52R2325"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9555" prefix="IC">
<description>&lt;b&gt;16-bit I2C and SMBus I/O port with interrupt&lt;/b&gt;&lt;p&gt;
Source: PCA9555_5.pdf</description>
<gates>
<gate name="G$1" symbol="PCA9555"/>
</gates>
<devices>
<device name="N" package="DIL24-6">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="I/O0.0" pad="4"/>
<connect gate="G$1" pin="I/O0.1" pad="5"/>
<connect gate="G$1" pin="I/O0.2" pad="6"/>
<connect gate="G$1" pin="I/O0.3" pad="7"/>
<connect gate="G$1" pin="I/O0.4" pad="8"/>
<connect gate="G$1" pin="I/O0.5" pad="9"/>
<connect gate="G$1" pin="I/O0.6" pad="10"/>
<connect gate="G$1" pin="I/O0.7" pad="11"/>
<connect gate="G$1" pin="I/O1.0" pad="13"/>
<connect gate="G$1" pin="I/O1.1" pad="14"/>
<connect gate="G$1" pin="I/O1.2" pad="15"/>
<connect gate="G$1" pin="I/O1.3" pad="16"/>
<connect gate="G$1" pin="I/O1.4" pad="17"/>
<connect gate="G$1" pin="I/O1.5" pad="18"/>
<connect gate="G$1" pin="I/O1.6" pad="19"/>
<connect gate="G$1" pin="I/O1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9555N,112"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R6677"/>
</technology>
</technologies>
</device>
<device name="D" package="SO24">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="I/O0.0" pad="4"/>
<connect gate="G$1" pin="I/O0.1" pad="5"/>
<connect gate="G$1" pin="I/O0.2" pad="6"/>
<connect gate="G$1" pin="I/O0.3" pad="7"/>
<connect gate="G$1" pin="I/O0.4" pad="8"/>
<connect gate="G$1" pin="I/O0.5" pad="9"/>
<connect gate="G$1" pin="I/O0.6" pad="10"/>
<connect gate="G$1" pin="I/O0.7" pad="11"/>
<connect gate="G$1" pin="I/O1.0" pad="13"/>
<connect gate="G$1" pin="I/O1.1" pad="14"/>
<connect gate="G$1" pin="I/O1.2" pad="15"/>
<connect gate="G$1" pin="I/O1.3" pad="16"/>
<connect gate="G$1" pin="I/O1.4" pad="17"/>
<connect gate="G$1" pin="I/O1.5" pad="18"/>
<connect gate="G$1" pin="I/O1.6" pad="19"/>
<connect gate="G$1" pin="I/O1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9555DW"/>
<attribute name="OC_FARNELL" value="1408295"/>
<attribute name="OC_NEWARK" value="63K6067"/>
</technology>
</technologies>
</device>
<device name="DB" package="SSOP24">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="I/O0.0" pad="4"/>
<connect gate="G$1" pin="I/O0.1" pad="5"/>
<connect gate="G$1" pin="I/O0.2" pad="6"/>
<connect gate="G$1" pin="I/O0.3" pad="7"/>
<connect gate="G$1" pin="I/O0.4" pad="8"/>
<connect gate="G$1" pin="I/O0.5" pad="9"/>
<connect gate="G$1" pin="I/O0.6" pad="10"/>
<connect gate="G$1" pin="I/O0.7" pad="11"/>
<connect gate="G$1" pin="I/O1.0" pad="13"/>
<connect gate="G$1" pin="I/O1.1" pad="14"/>
<connect gate="G$1" pin="I/O1.2" pad="15"/>
<connect gate="G$1" pin="I/O1.3" pad="16"/>
<connect gate="G$1" pin="I/O1.4" pad="17"/>
<connect gate="G$1" pin="I/O1.5" pad="18"/>
<connect gate="G$1" pin="I/O1.6" pad="19"/>
<connect gate="G$1" pin="I/O1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9555DB"/>
<attribute name="OC_FARNELL" value="1408295"/>
<attribute name="OC_NEWARK" value="63K6063"/>
</technology>
</technologies>
</device>
<device name="BS" package="HVQFN24">
<connects>
<connect gate="G$1" pin="!INT" pad="22"/>
<connect gate="G$1" pin="A0" pad="18"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A2" pad="24"/>
<connect gate="G$1" pin="I/O0.0" pad="1"/>
<connect gate="G$1" pin="I/O0.1" pad="2"/>
<connect gate="G$1" pin="I/O0.2" pad="3"/>
<connect gate="G$1" pin="I/O0.3" pad="4"/>
<connect gate="G$1" pin="I/O0.4" pad="5"/>
<connect gate="G$1" pin="I/O0.5" pad="6"/>
<connect gate="G$1" pin="I/O0.6" pad="7"/>
<connect gate="G$1" pin="I/O0.7" pad="8"/>
<connect gate="G$1" pin="I/O1.0" pad="10"/>
<connect gate="G$1" pin="I/O1.1" pad="11"/>
<connect gate="G$1" pin="I/O1.2" pad="12"/>
<connect gate="G$1" pin="I/O1.3" pad="13"/>
<connect gate="G$1" pin="I/O1.4" pad="14"/>
<connect gate="G$1" pin="I/O1.5" pad="15"/>
<connect gate="G$1" pin="I/O1.6" pad="16"/>
<connect gate="G$1" pin="I/O1.7" pad="17"/>
<connect gate="G$1" pin="SCL" pad="19"/>
<connect gate="G$1" pin="SDA" pad="20"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VSS" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9555BS,118"/>
<attribute name="OC_FARNELL" value="1575354"/>
<attribute name="OC_NEWARK" value="70R6671"/>
</technology>
</technologies>
</device>
<device name="PW" package="TSSOP24">
<connects>
<connect gate="G$1" pin="!INT" pad="1"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="I/O0.0" pad="4"/>
<connect gate="G$1" pin="I/O0.1" pad="5"/>
<connect gate="G$1" pin="I/O0.2" pad="6"/>
<connect gate="G$1" pin="I/O0.3" pad="7"/>
<connect gate="G$1" pin="I/O0.4" pad="8"/>
<connect gate="G$1" pin="I/O0.5" pad="9"/>
<connect gate="G$1" pin="I/O0.6" pad="10"/>
<connect gate="G$1" pin="I/O0.7" pad="11"/>
<connect gate="G$1" pin="I/O1.0" pad="13"/>
<connect gate="G$1" pin="I/O1.1" pad="14"/>
<connect gate="G$1" pin="I/O1.2" pad="15"/>
<connect gate="G$1" pin="I/O1.3" pad="16"/>
<connect gate="G$1" pin="I/O1.4" pad="17"/>
<connect gate="G$1" pin="I/O1.5" pad="18"/>
<connect gate="G$1" pin="I/O1.6" pad="19"/>
<connect gate="G$1" pin="I/O1.7" pad="20"/>
<connect gate="G$1" pin="SCL" pad="22"/>
<connect gate="G$1" pin="SDA" pad="23"/>
<connect gate="G$1" pin="VDD" pad="24"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9555PW"/>
<attribute name="OC_FARNELL" value="1408297"/>
<attribute name="OC_NEWARK" value="63K6069"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PN531" prefix="IC">
<description>&lt;b&gt;Near Field Communication Transmission module&lt;/b&gt;&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/other/identification/sfs_pn531_rev2.0.pdf</description>
<gates>
<gate name="G$1" symbol="PN531"/>
</gates>
<devices>
<device name="" package="HVQFN40">
<connects>
<connect gate="G$1" pin="!RSTOUT" pad="29"/>
<connect gate="G$1" pin="!RSTPD" pad="38"/>
<connect gate="G$1" pin="AUX1" pad="12"/>
<connect gate="G$1" pin="AUX2" pad="13"/>
<connect gate="G$1" pin="AVDD" pad="8"/>
<connect gate="G$1" pin="AVSS" pad="11"/>
<connect gate="G$1" pin="DELATT" pad="30"/>
<connect gate="G$1" pin="DVDD" pad="39"/>
<connect gate="G$1" pin="DVSS" pad="1"/>
<connect gate="G$1" pin="I0" pad="16"/>
<connect gate="G$1" pin="I1" pad="17"/>
<connect gate="G$1" pin="IRQ" pad="28"/>
<connect gate="G$1" pin="LOADMOD" pad="2"/>
<connect gate="G$1" pin="MISO" pad="33"/>
<connect gate="G$1" pin="MOSI" pad="32"/>
<connect gate="G$1" pin="NSS" pad="31"/>
<connect gate="G$1" pin="OSC2IN" pad="20"/>
<connect gate="G$1" pin="OSC2OUT" pad="19"/>
<connect gate="G$1" pin="OSCIN" pad="14"/>
<connect gate="G$1" pin="OSCOUT" pad="15"/>
<connect gate="G$1" pin="P30" pad="27"/>
<connect gate="G$1" pin="P31" pad="26"/>
<connect gate="G$1" pin="P32_INT0" pad="37"/>
<connect gate="G$1" pin="P33_INT1" pad="36"/>
<connect gate="G$1" pin="P34" pad="22"/>
<connect gate="G$1" pin="P35" pad="21"/>
<connect gate="G$1" pin="PVDD" pad="35"/>
<connect gate="G$1" pin="RX" pad="10"/>
<connect gate="G$1" pin="SCK" pad="34"/>
<connect gate="G$1" pin="SIGIN" pad="24"/>
<connect gate="G$1" pin="SIGOUT" pad="23"/>
<connect gate="G$1" pin="SVDD" pad="25"/>
<connect gate="G$1" pin="TESTEN" pad="18"/>
<connect gate="G$1" pin="TH" pad="TH"/>
<connect gate="G$1" pin="TVDD" pad="5"/>
<connect gate="G$1" pin="TVSS1" pad="3"/>
<connect gate="G$1" pin="TVSS2" pad="7"/>
<connect gate="G$1" pin="TX1" pad="4"/>
<connect gate="G$1" pin="TX2" pad="6"/>
<connect gate="G$1" pin="VBUS" pad="40"/>
<connect gate="G$1" pin="VMID" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PN5310A3HN/C203,51"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R7886"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEA5764HN" prefix="IC">
<description>&lt;b&gt;FM radio + RDS&lt;/b&gt;&lt;p&gt;
single chip electronically tuned FM stereo radio with Radio Data System (RDS)&lt;br&gt;
and Radio Broadcast Data System (RBDS) demodulator and RDS/RBDS decoder&lt;br&gt;
for portable application with fully integrated IF selectivity and demodulation.&lt;br&gt;
Source: http://www.nxp.com .. TEA5764HN_2.pdf</description>
<gates>
<gate name="G$1" symbol="TEA5764HN"/>
</gates>
<devices>
<device name="" package="HVQFN40">
<connects>
<connect gate="G$1" pin="BUSENBABLE" pad="8"/>
<connect gate="G$1" pin="CAGC" pad="39"/>
<connect gate="G$1" pin="CD1" pad="5"/>
<connect gate="G$1" pin="CD2/INTCON3" pad="16"/>
<connect gate="G$1" pin="CD3" pad="35"/>
<connect gate="G$1" pin="CPOUT" pad="2"/>
<connect gate="G$1" pin="FREQIN" pad="32"/>
<connect gate="G$1" pin="GNDA" pad="30"/>
<connect gate="G$1" pin="GNDD" pad="13"/>
<connect gate="G$1" pin="GNDD@1" pad="14"/>
<connect gate="G$1" pin="GNDD@2" pad="19"/>
<connect gate="G$1" pin="GNDD@3" pad="28"/>
<connect gate="G$1" pin="GNDRF" pad="38"/>
<connect gate="G$1" pin="INTCON1" pad="22"/>
<connect gate="G$1" pin="INTCON2" pad="18"/>
<connect gate="G$1" pin="INTX" pad="20"/>
<connect gate="G$1" pin="LO1" pad="3"/>
<connect gate="G$1" pin="LO2" pad="4"/>
<connect gate="G$1" pin="LOOPSW" pad="1"/>
<connect gate="G$1" pin="MPXIN" pad="27"/>
<connect gate="G$1" pin="MPXOUT" pad="26"/>
<connect gate="G$1" pin="PILLP" pad="6"/>
<connect gate="G$1" pin="RFIN1" pad="36"/>
<connect gate="G$1" pin="RFIN2" pad="37"/>
<connect gate="G$1" pin="SCL" pad="10"/>
<connect gate="G$1" pin="SDA" pad="11"/>
<connect gate="G$1" pin="SWPORT" pad="7"/>
<connect gate="G$1" pin="TH" pad="TH"/>
<connect gate="G$1" pin="TMUTE" pad="23"/>
<connect gate="G$1" pin="VAFL" pad="25"/>
<connect gate="G$1" pin="VAFR" pad="24"/>
<connect gate="G$1" pin="VCCA" pad="34"/>
<connect gate="G$1" pin="VCCD" pad="15"/>
<connect gate="G$1" pin="VREFDIG" pad="9"/>
<connect gate="G$1" pin="XTAL" pad="33"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P98LPC935" prefix="IC">
<description>&lt;b&gt;8-bit microcontroller with accelerated two-clock core&lt;/b&gt;&lt;p&gt;
4 KB/ 8 KB/ 8 KB 3 V byte-erasable Flash with 8-bit A/D converter&lt;br&gt;
Source: http://www.nxp.com .. UM_P89LPC933_934_935_1.pdf</description>
<gates>
<gate name="G$1" symbol="P98LPC935"/>
</gates>
<devices>
<device name="P" package="DIL28">
<connects>
<connect gate="G$1" pin="!INT1/P1.4" pad="10"/>
<connect gate="G$1" pin="!RST/P1.5" pad="6"/>
<connect gate="G$1" pin="AD00/P1.7" pad="4"/>
<connect gate="G$1" pin="AD01/P2.0" pad="3"/>
<connect gate="G$1" pin="AD02/P2.1" pad="2"/>
<connect gate="G$1" pin="AD03/DAC0/P2.0" pad="1"/>
<connect gate="G$1" pin="CLKOUT/XTAL2/P3.0" pad="9"/>
<connect gate="G$1" pin="MISO/P2.3" pad="14"/>
<connect gate="G$1" pin="MOSI/P2.2" pad="13"/>
<connect gate="G$1" pin="OCB/P1.6" pad="5"/>
<connect gate="G$1" pin="P0.1/CIN2B/AD10" pad="26"/>
<connect gate="G$1" pin="P0.2/CIN2A/AD11" pad="25"/>
<connect gate="G$1" pin="P0.3/CIN1B/AD12" pad="24"/>
<connect gate="G$1" pin="P0.4/CIN1A/DAC1/AD13" pad="23"/>
<connect gate="G$1" pin="P0.5/CMPREF" pad="22"/>
<connect gate="G$1" pin="P0.6/CMP1" pad="20"/>
<connect gate="G$1" pin="P0.7/T1" pad="19"/>
<connect gate="G$1" pin="P1.0/TXD" pad="18"/>
<connect gate="G$1" pin="P1.1/RXD" pad="17"/>
<connect gate="G$1" pin="P2.4/!SS" pad="15"/>
<connect gate="G$1" pin="P2.5/SPICLK" pad="16"/>
<connect gate="G$1" pin="P2.6/OCA" pad="27"/>
<connect gate="G$1" pin="P2.7/ICA" pad="28"/>
<connect gate="G$1" pin="SCL/T0/P1.2" pad="12"/>
<connect gate="G$1" pin="SDA/!INT0/P1.2" pad="11"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="XTAL1/P3.1" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="PLCC28S">
<connects>
<connect gate="G$1" pin="!INT1/P1.4" pad="10"/>
<connect gate="G$1" pin="!RST/P1.5" pad="6"/>
<connect gate="G$1" pin="AD00/P1.7" pad="4"/>
<connect gate="G$1" pin="AD01/P2.0" pad="3"/>
<connect gate="G$1" pin="AD02/P2.1" pad="2"/>
<connect gate="G$1" pin="AD03/DAC0/P2.0" pad="1"/>
<connect gate="G$1" pin="CLKOUT/XTAL2/P3.0" pad="9"/>
<connect gate="G$1" pin="MISO/P2.3" pad="14"/>
<connect gate="G$1" pin="MOSI/P2.2" pad="13"/>
<connect gate="G$1" pin="OCB/P1.6" pad="5"/>
<connect gate="G$1" pin="P0.1/CIN2B/AD10" pad="26"/>
<connect gate="G$1" pin="P0.2/CIN2A/AD11" pad="25"/>
<connect gate="G$1" pin="P0.3/CIN1B/AD12" pad="24"/>
<connect gate="G$1" pin="P0.4/CIN1A/DAC1/AD13" pad="23"/>
<connect gate="G$1" pin="P0.5/CMPREF" pad="22"/>
<connect gate="G$1" pin="P0.6/CMP1" pad="20"/>
<connect gate="G$1" pin="P0.7/T1" pad="19"/>
<connect gate="G$1" pin="P1.0/TXD" pad="18"/>
<connect gate="G$1" pin="P1.1/RXD" pad="17"/>
<connect gate="G$1" pin="P2.4/!SS" pad="15"/>
<connect gate="G$1" pin="P2.5/SPICLK" pad="16"/>
<connect gate="G$1" pin="P2.6/OCA" pad="27"/>
<connect gate="G$1" pin="P2.7/ICA" pad="28"/>
<connect gate="G$1" pin="SCL/T0/P1.2" pad="12"/>
<connect gate="G$1" pin="SDA/!INT0/P1.2" pad="11"/>
<connect gate="G$1" pin="VDD" pad="21"/>
<connect gate="G$1" pin="VSS" pad="7"/>
<connect gate="G$1" pin="XTAL1/P3.1" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="H" package="HVQFN28">
<connects>
<connect gate="G$1" pin="!INT1/P1.4" pad="6"/>
<connect gate="G$1" pin="!RST/P1.5" pad="2"/>
<connect gate="G$1" pin="AD00/P1.7" pad="28"/>
<connect gate="G$1" pin="AD01/P2.0" pad="27"/>
<connect gate="G$1" pin="AD02/P2.1" pad="26"/>
<connect gate="G$1" pin="AD03/DAC0/P2.0" pad="25"/>
<connect gate="G$1" pin="CLKOUT/XTAL2/P3.0" pad="5"/>
<connect gate="G$1" pin="MISO/P2.3" pad="10"/>
<connect gate="G$1" pin="MOSI/P2.2" pad="9"/>
<connect gate="G$1" pin="OCB/P1.6" pad="1"/>
<connect gate="G$1" pin="P0.1/CIN2B/AD10" pad="22"/>
<connect gate="G$1" pin="P0.2/CIN2A/AD11" pad="21"/>
<connect gate="G$1" pin="P0.3/CIN1B/AD12" pad="20"/>
<connect gate="G$1" pin="P0.4/CIN1A/DAC1/AD13" pad="19"/>
<connect gate="G$1" pin="P0.5/CMPREF" pad="18"/>
<connect gate="G$1" pin="P0.6/CMP1" pad="16"/>
<connect gate="G$1" pin="P0.7/T1" pad="15"/>
<connect gate="G$1" pin="P1.0/TXD" pad="14"/>
<connect gate="G$1" pin="P1.1/RXD" pad="13"/>
<connect gate="G$1" pin="P2.4/!SS" pad="11"/>
<connect gate="G$1" pin="P2.5/SPICLK" pad="12"/>
<connect gate="G$1" pin="P2.6/OCA" pad="23"/>
<connect gate="G$1" pin="P2.7/ICA" pad="24"/>
<connect gate="G$1" pin="SCL/T0/P1.2" pad="8"/>
<connect gate="G$1" pin="SDA/!INT0/P1.2" pad="7"/>
<connect gate="G$1" pin="VDD" pad="17"/>
<connect gate="G$1" pin="VSS" pad="3"/>
<connect gate="G$1" pin="XTAL1/P3.1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9505" prefix="IC">
<description>&lt;b&gt;40-bit I2C-bus I/O port with /RESET, /OE and /INT&lt;/b&gt;&lt;p&gt;
The 9505 has 100k ohm pull-ups on IO pins.&lt;br&gt;
Source: http://www.nxp.com/acrobat_download/datasheets/PCA9505_9506_3.pdf</description>
<gates>
<gate name="G$1" symbol="PCA9505"/>
</gates>
<devices>
<device name="" package="TSSOP56-6">
<connects>
<connect gate="G$1" pin="!INT" pad="55"/>
<connect gate="G$1" pin="!OE" pad="30"/>
<connect gate="G$1" pin="!RESET" pad="56"/>
<connect gate="G$1" pin="A0" pad="27"/>
<connect gate="G$1" pin="A1" pad="28"/>
<connect gate="G$1" pin="A2" pad="29"/>
<connect gate="G$1" pin="IO0_0" pad="3"/>
<connect gate="G$1" pin="IO0_1" pad="4"/>
<connect gate="G$1" pin="IO0_2" pad="5"/>
<connect gate="G$1" pin="IO0_3" pad="7"/>
<connect gate="G$1" pin="IO0_4" pad="8"/>
<connect gate="G$1" pin="IO0_5" pad="9"/>
<connect gate="G$1" pin="IO0_6" pad="10"/>
<connect gate="G$1" pin="IO0_7" pad="12"/>
<connect gate="G$1" pin="IO1_0" pad="13"/>
<connect gate="G$1" pin="IO1_1" pad="14"/>
<connect gate="G$1" pin="IO1_2" pad="15"/>
<connect gate="G$1" pin="IO1_3" pad="16"/>
<connect gate="G$1" pin="IO1_4" pad="17"/>
<connect gate="G$1" pin="IO1_5" pad="19"/>
<connect gate="G$1" pin="IO1_6" pad="20"/>
<connect gate="G$1" pin="IO1_7" pad="21"/>
<connect gate="G$1" pin="IO2_0" pad="22"/>
<connect gate="G$1" pin="IO2_1" pad="24"/>
<connect gate="G$1" pin="IO2_2" pad="25"/>
<connect gate="G$1" pin="IO2_3" pad="26"/>
<connect gate="G$1" pin="IO2_4" pad="31"/>
<connect gate="G$1" pin="IO2_5" pad="32"/>
<connect gate="G$1" pin="IO2_6" pad="33"/>
<connect gate="G$1" pin="IO2_7" pad="35"/>
<connect gate="G$1" pin="IO3_0" pad="36"/>
<connect gate="G$1" pin="IO3_1" pad="37"/>
<connect gate="G$1" pin="IO3_2" pad="38"/>
<connect gate="G$1" pin="IO3_3" pad="40"/>
<connect gate="G$1" pin="IO3_4" pad="41"/>
<connect gate="G$1" pin="IO3_5" pad="42"/>
<connect gate="G$1" pin="IO3_6" pad="43"/>
<connect gate="G$1" pin="IO3_7" pad="44"/>
<connect gate="G$1" pin="IO4_0" pad="45"/>
<connect gate="G$1" pin="IO4_1" pad="47"/>
<connect gate="G$1" pin="IO4_2" pad="48"/>
<connect gate="G$1" pin="IO4_3" pad="49"/>
<connect gate="G$1" pin="IO4_4" pad="50"/>
<connect gate="G$1" pin="IO4_5" pad="52"/>
<connect gate="G$1" pin="IO4_6" pad="53"/>
<connect gate="G$1" pin="IO4_7" pad="54"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="18"/>
<connect gate="G$1" pin="VDD@2" pad="46"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="11"/>
<connect gate="G$1" pin="VSS@3" pad="23"/>
<connect gate="G$1" pin="VSS@4" pad="34"/>
<connect gate="G$1" pin="VSS@5" pad="39"/>
<connect gate="G$1" pin="VSS@6" pad="51"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9505DGG,118"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R6450"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9506">
<description>40-bit I2C-bus I/O port with /RESET, /OE and /INT

The 9506 has no pull-ups on IO pins.

Source:  http://www.nxp.com/acrobat_download/datasheets/PCA9505_9506_3.pdf</description>
<gates>
<gate name="G$1" symbol="PCA9506"/>
</gates>
<devices>
<device name="" package="TSSOP56-6">
<connects>
<connect gate="G$1" pin="!INT" pad="55"/>
<connect gate="G$1" pin="!OE" pad="30"/>
<connect gate="G$1" pin="!RESET" pad="56"/>
<connect gate="G$1" pin="A0" pad="27"/>
<connect gate="G$1" pin="A1" pad="28"/>
<connect gate="G$1" pin="A2" pad="29"/>
<connect gate="G$1" pin="IO0_0" pad="3"/>
<connect gate="G$1" pin="IO0_1" pad="4"/>
<connect gate="G$1" pin="IO0_2" pad="5"/>
<connect gate="G$1" pin="IO0_3" pad="7"/>
<connect gate="G$1" pin="IO0_4" pad="8"/>
<connect gate="G$1" pin="IO0_5" pad="9"/>
<connect gate="G$1" pin="IO0_6" pad="10"/>
<connect gate="G$1" pin="IO0_7" pad="12"/>
<connect gate="G$1" pin="IO1_0" pad="13"/>
<connect gate="G$1" pin="IO1_1" pad="14"/>
<connect gate="G$1" pin="IO1_2" pad="15"/>
<connect gate="G$1" pin="IO1_3" pad="16"/>
<connect gate="G$1" pin="IO1_4" pad="17"/>
<connect gate="G$1" pin="IO1_5" pad="19"/>
<connect gate="G$1" pin="IO1_6" pad="20"/>
<connect gate="G$1" pin="IO1_7" pad="21"/>
<connect gate="G$1" pin="IO2_0" pad="22"/>
<connect gate="G$1" pin="IO2_1" pad="24"/>
<connect gate="G$1" pin="IO2_2" pad="25"/>
<connect gate="G$1" pin="IO2_3" pad="26"/>
<connect gate="G$1" pin="IO2_4" pad="31"/>
<connect gate="G$1" pin="IO2_5" pad="32"/>
<connect gate="G$1" pin="IO2_6" pad="33"/>
<connect gate="G$1" pin="IO2_7" pad="35"/>
<connect gate="G$1" pin="IO3_0" pad="36"/>
<connect gate="G$1" pin="IO3_1" pad="37"/>
<connect gate="G$1" pin="IO3_2" pad="38"/>
<connect gate="G$1" pin="IO3_3" pad="40"/>
<connect gate="G$1" pin="IO3_4" pad="41"/>
<connect gate="G$1" pin="IO3_5" pad="42"/>
<connect gate="G$1" pin="IO3_6" pad="43"/>
<connect gate="G$1" pin="IO3_7" pad="44"/>
<connect gate="G$1" pin="IO4_0" pad="45"/>
<connect gate="G$1" pin="IO4_1" pad="47"/>
<connect gate="G$1" pin="IO4_2" pad="48"/>
<connect gate="G$1" pin="IO4_3" pad="49"/>
<connect gate="G$1" pin="IO4_4" pad="50"/>
<connect gate="G$1" pin="IO4_5" pad="52"/>
<connect gate="G$1" pin="IO4_6" pad="53"/>
<connect gate="G$1" pin="IO4_7" pad="54"/>
<connect gate="G$1" pin="SCL" pad="2"/>
<connect gate="G$1" pin="SDA" pad="1"/>
<connect gate="G$1" pin="VDD@1" pad="18"/>
<connect gate="G$1" pin="VDD@2" pad="46"/>
<connect gate="G$1" pin="VSS@1" pad="6"/>
<connect gate="G$1" pin="VSS@2" pad="11"/>
<connect gate="G$1" pin="VSS@3" pad="23"/>
<connect gate="G$1" pin="VSS@4" pad="34"/>
<connect gate="G$1" pin="VSS@5" pad="39"/>
<connect gate="G$1" pin="VSS@6" pad="51"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9506DGG,512"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R6452"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCA9534" prefix="IC">
<description>&lt;b&gt;8-bit I2C-bus and SMBus low power I/O port with interrupt&lt;/b&gt;&lt;p&gt;
Source: www.nxp.com .. PCA9534_3.pdf</description>
<gates>
<gate name="P" symbol="PCA9534"/>
</gates>
<devices>
<device name="PW" package="TSSOP16">
<connects>
<connect gate="P" pin="!INT" pad="13"/>
<connect gate="P" pin="A0" pad="1"/>
<connect gate="P" pin="A1" pad="2"/>
<connect gate="P" pin="A2" pad="3"/>
<connect gate="P" pin="IO0" pad="4"/>
<connect gate="P" pin="IO1" pad="5"/>
<connect gate="P" pin="IO2" pad="6"/>
<connect gate="P" pin="IO3" pad="7"/>
<connect gate="P" pin="IO4" pad="9"/>
<connect gate="P" pin="IO5" pad="10"/>
<connect gate="P" pin="IO6" pad="11"/>
<connect gate="P" pin="IO7" pad="12"/>
<connect gate="P" pin="SCL" pad="14"/>
<connect gate="P" pin="SDA" pad="15"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9534PW"/>
<attribute name="OC_FARNELL" value="1408285"/>
<attribute name="OC_NEWARK" value="18M7516"/>
</technology>
</technologies>
</device>
<device name="D" package="SO16W">
<connects>
<connect gate="P" pin="!INT" pad="13"/>
<connect gate="P" pin="A0" pad="1"/>
<connect gate="P" pin="A1" pad="2"/>
<connect gate="P" pin="A2" pad="3"/>
<connect gate="P" pin="IO0" pad="4"/>
<connect gate="P" pin="IO1" pad="5"/>
<connect gate="P" pin="IO2" pad="6"/>
<connect gate="P" pin="IO3" pad="7"/>
<connect gate="P" pin="IO4" pad="9"/>
<connect gate="P" pin="IO5" pad="10"/>
<connect gate="P" pin="IO6" pad="11"/>
<connect gate="P" pin="IO7" pad="12"/>
<connect gate="P" pin="SCL" pad="14"/>
<connect gate="P" pin="SDA" pad="15"/>
<connect gate="P" pin="VDD" pad="16"/>
<connect gate="P" pin="VSS" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9534DB"/>
<attribute name="OC_FARNELL" value="1408284"/>
<attribute name="OC_NEWARK" value="18M7513"/>
</technology>
</technologies>
</device>
<device name="BS" package="HVQFN16_4X4">
<connects>
<connect gate="P" pin="!INT" pad="11"/>
<connect gate="P" pin="A0" pad="15"/>
<connect gate="P" pin="A1" pad="16"/>
<connect gate="P" pin="A2" pad="1"/>
<connect gate="P" pin="IO0" pad="2"/>
<connect gate="P" pin="IO1" pad="3"/>
<connect gate="P" pin="IO2" pad="4"/>
<connect gate="P" pin="IO3" pad="5"/>
<connect gate="P" pin="IO4" pad="7"/>
<connect gate="P" pin="IO5" pad="8"/>
<connect gate="P" pin="IO6" pad="9"/>
<connect gate="P" pin="IO7" pad="10"/>
<connect gate="P" pin="SCL" pad="12"/>
<connect gate="P" pin="SDA" pad="13"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9534BS,118"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R6525"/>
</technology>
</technologies>
</device>
<device name="BS3" package="HVQFN16_3X3">
<connects>
<connect gate="P" pin="!INT" pad="11"/>
<connect gate="P" pin="A0" pad="15"/>
<connect gate="P" pin="A1" pad="16"/>
<connect gate="P" pin="A2" pad="1"/>
<connect gate="P" pin="IO0" pad="2"/>
<connect gate="P" pin="IO1" pad="3"/>
<connect gate="P" pin="IO2" pad="4"/>
<connect gate="P" pin="IO3" pad="5"/>
<connect gate="P" pin="IO4" pad="7"/>
<connect gate="P" pin="IO5" pad="8"/>
<connect gate="P" pin="IO6" pad="9"/>
<connect gate="P" pin="IO7" pad="10"/>
<connect gate="P" pin="SCL" pad="12"/>
<connect gate="P" pin="SDA" pad="13"/>
<connect gate="P" pin="VDD" pad="14"/>
<connect gate="P" pin="VSS" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCA9534BS3,118"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70R6526"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LPC1102" prefix="IC">
<description>&lt;b&gt;32-bit ARM Cortex-M0 microcontroller; 32 kB flash and 8 kB SRAM&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://ics.nxp.com/products/lpc1000/datasheet/lpc1102.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LPC1102"/>
</gates>
<devices>
<device name="" package="WLCSP16">
<connects>
<connect gate="G$1" pin="PIO0_8/MISO/CT16B0_MAT0" pad="A2"/>
<connect gate="G$1" pin="PIO0_9/MOSI/CT16B0_MAT1" pad="A3"/>
<connect gate="G$1" pin="PIO1_6/RXD/CT32B0_MAT0" pad="C2"/>
<connect gate="G$1" pin="PIO1_7/TXD/CT32B0_MAT1" pad="D1"/>
<connect gate="G$1" pin="R/PIO0_11/AD0/CT32B0_MAT3" pad="B4"/>
<connect gate="G$1" pin="R/PIO1_0/AD1/CT32B1_CAP0" pad="B3"/>
<connect gate="G$1" pin="R/PIO1_1/AD2/CT32B1_MAT0" pad="C4"/>
<connect gate="G$1" pin="R/PIO1_2/AD3/CT32B1_MAT1" pad="C3"/>
<connect gate="G$1" pin="RESET/PIO0_0" pad="C1"/>
<connect gate="G$1" pin="SWCLK/PIO0_10/SCK/CT16B0_MAT2" pad="A4"/>
<connect gate="G$1" pin="SWDIO/PIO1_3/AD4/CT32B1_MAT2" pad="D4"/>
<connect gate="G$1" pin="VDD" pad="A1"/>
<connect gate="G$1" pin="VDD@1" pad="D2"/>
<connect gate="G$1" pin="VSS" pad="B1"/>
<connect gate="G$1" pin="VSS@1" pad="D3"/>
<connect gate="G$1" pin="XTALIN" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
