<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Siemens Microcontroller and Microprocessor Devices&lt;/b&gt;&lt;p&gt;
www.siemens.de&lt;p&gt;
Devices included from Alex Bluemel&lt;br&gt;
8*C535.DEV&lt;br&gt;
BTS428L2.DEV&lt;br&gt;
BTS555.DEV&lt;br&gt;
SA*-C161CS.DEV&lt;br&gt;
SA*-C165-RF.DEV&lt;br&gt;
SA*-C165-RM.DEV&lt;br&gt;
SA*-C167-LM.DEV&lt;br&gt;
SA*-C167CR-LM.DEV&lt;br&gt;
SA*-XC167.DEV&lt;br&gt;
SA*-XC167CI.DEV&lt;br&gt;
SA*C167-CR-LM.DEV&lt;br&gt;
SAF-XC2264.DEV&lt;br&gt;
SAK-TC1100*.DEV&lt;br&gt;
SAK-TC1130*.DEV&lt;br&gt;
SAK-TC1762*.DEV&lt;br&gt;
SAK-TC1796.DEV&lt;br&gt;
SAK-TC1910*.DEV&lt;br&gt;
SAK-TC1920*.DEV&lt;br&gt;
TC-10.DEV&lt;br&gt;
TC10.DEV&lt;br&gt;
TC11IB.DEV&lt;br&gt;
TC191*.DEV&lt;br&gt;
TC1100.DEV&lt;br&gt;
TC1130.DEV&lt;br&gt;
TC1762.DEV&lt;br&gt;
TC1765.DEV&lt;br&gt;
TC1775.DEV&lt;br&gt;
TC1920.DEV&lt;br&gt;
TDA6060*.DEV&lt;br&gt;
TLE6361G.DEV&lt;br&gt;
XC167.DEV&lt;br&gt;
&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MQFP100">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="MQFP80-2">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="MQFP80-1">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="MQFP64-1">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="MQFP44-2">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="MQFP144">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="MQFP160">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP48">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP64">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP100">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP128">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP144">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP176">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP184">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="FQFP208">
<description>&lt;b&gt;Fine Pitch Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="BQFP100">
<description>&lt;b&gt;Bumpered Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="CQFP-84">
<description>&lt;b&gt;Ceramic Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="MQUAD144">
<description>&lt;b&gt;Metal Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="MQUAD160">
<description>&lt;b&gt;Metal Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PLCC68">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="PGA68">
<description>&lt;b&gt;Pin Grid Array&lt;/b&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="PLCC84">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="TO220511">
<description>&lt;b&gt;Transistor Outline Package&lt;/b&gt; P-TO220-5-11</description>
</package>
<package name="TO220512">
<description>&lt;b&gt;Transistor Outline Package&lt;/b&gt; P-TO220-5-12</description>
</package>
<package name="TO263-51">
<description>&lt;b&gt;Transistor Outline Package&lt;/b&gt; P-TO263-5-1</description>
</package>
<package name="TO220-58">
<description>&lt;b&gt;Transistor Outline Package&lt;/b&gt; P-TO220-5-8</description>
</package>
<package name="TO252-51">
<description>&lt;b&gt;Transistor Outline Package&lt;/b&gt; P-TO252-5-1</description>
</package>
<package name="PDSO_20-9">
<description>&lt;b&gt;Plastic Small Outline&lt;/b&gt;</description>
</package>
<package name="PLCC68SOCK">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
socked</description>
</package>
<package name="PDSO_36-12">
<description>&lt;b&gt;Plastic Small Outline&lt;/b&gt;</description>
</package>
<package name="PGA145">
<description>&lt;b&gt;S-PGA-15-145-A&lt;/b&gt;&lt;p&gt;
Emulation Technology, Inc.</description>
</package>
<package name="PGA145S">
<description>&lt;b&gt;S-PGA-15-145-AZ&lt;/b&gt; SOCKED&lt;p&gt;
Emulation Technology, Inc.</description>
</package>
<package name="PBGA217">
<description>&lt;b&gt;PBGA 217&lt;/b&gt;</description>
</package>
<package name="PLCC84SOCK">
<description>&lt;b&gt;PLCC 84 socked&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL40">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="DIL22-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="QFP100R">
<description>&lt;b&gt;Quad Flat Pack Package&lt;/b&gt; 100 Pin Rectangle&lt;p&gt;
Source: Siemens dpc31_d.pdf</description>
</package>
<package name="TO252-5-11">
<description>&lt;b&gt;Dpak-5 Pin&lt;/b&gt; P-TO252-5-11 &lt;/b&gt;&lt;p&gt;
Source: www.infineon.com .. BTS428L2_20030912.pdf</description>
</package>
<package name="TO220-51">
<description>&lt;b&gt;TO-218AB/5-1&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/upload/Document/cmc_upload/documents/011/8726/Datasheet_BTS555.pdf</description>
</package>
<package name="TO220-52">
<description>&lt;b&gt;TO-218AB/5 Option E3146&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/upload/Document/cmc_upload/documents/011/8726/Datasheet_BTS555.pdf</description>
</package>
<package name="P-TQFP-128">
<description>&lt;b&gt;P-TQFP-128 with rounded pads&lt;/b&gt;</description>
</package>
<package name="MQFP144-RND">
<description>&lt;b&gt;Metric Quad Flat Pack&lt;/b&gt; with rounded pads</description>
</package>
<package name="P-TQFP-144-19">
<description>&lt;b&gt;P-TQFP-144-19 &lt;/b Plastic Metric Quad Flat Package&lt;p&gt;
Source: http://www.infineon.com/cgi/ecrm.dll/ecrm/scripts/pack_ov.jsp?oid=23155&amp;cat_oid=-8823</description>
</package>
<package name="P-TQFP144">
<description>&lt;b&gt;P-TQFP144 with rounded pads&lt;/b&gt;</description>
</package>
<package name="P-LBGA-208-2">
<description>&lt;b&gt;P-LBGA-208-2&lt;/b&gt; Low Profile Plastic Ball Grid Array Package&lt;p&gt;
Source: http://www.infineon.com .. TC1130_DS_v031.pdf</description>
</package>
<package name="P-LQFP-176-2">
<description>&lt;b&gt;P-LQFP-176-2 with rounded pads&lt;/b&gt;</description>
</package>
<package name="P-BGA-416">
<description>&lt;b&gt; P-BGA-416 Plastic Low Profile Pitch Ball Grid Array&lt;/b&gt;</description>
</package>
<package name="P-LBGA-260">
<description>&lt;b&gt;P-LBGA-260&lt;/b&gt; Plastic Ball Grid Array Package&lt;p&gt;
Source: http://www.infineon.com</description>
</package>
<package name="FQFP208-2">
<description>&lt;b&gt;P-FQFP-208-2, -4, -7&lt;/b&gt; Plastic Fine Pitch Quad Flat Package&lt;p&gt;
Source: http://www.infineon.com</description>
</package>
<package name="P-BGA-388-2">
<description>&lt;b&gt;P-BGA-388&lt;/b&gt; Plastic Ball Grid Array Package&lt;p&gt;
Source: www.infenon.com .. gpa09218.eps.ps</description>
</package>
<package name="P-BGA329">
<description>&lt;b&gt;P-BGA-329&lt;/b&gt; Plastic Ball Grid Array Package&lt;p&gt;
Source: http://www.infineon.com</description>
</package>
<package name="P-TSSOP28-1">
<description>Infineon &lt;b&gt;P-TSSOP-28-1&lt;/b&gt;&lt;p&gt;
TDA 6060 XS cross-ref_pFET-60v_p_chan.pdf</description>
</package>
<package name="DSO36">
<description>&lt;b&gt;DSO36&lt;/b&gt;
Source: TLE6361G</description>
</package>
</packages>
<symbols>
<symbol name="80C166">
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P0-8"/>
<pin name="P0-9"/>
<pin name="P0-10"/>
<pin name="P0-11"/>
<pin name="P0-12"/>
<pin name="P0-13"/>
<pin name="P0-14"/>
<pin name="P0-15"/>
<pin name="P0-0"/>
<pin name="P5-0" direction="in"/>
<pin name="P5-1" direction="in"/>
<pin name="P5-2" direction="in"/>
<pin name="P5-3" direction="in"/>
<pin name="P5-4" direction="in"/>
<pin name="P5-5" direction="in"/>
<pin name="P5-6" direction="in"/>
<pin name="P5-7" direction="in"/>
<pin name="P5-8" direction="in"/>
<pin name="P5-9" direction="in"/>
<pin name="P1-0"/>
<pin name="P1-1"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P1-8"/>
<pin name="P1-9"/>
<pin name="P1-10"/>
<pin name="P1-11"/>
<pin name="P1-12"/>
<pin name="P1-13"/>
<pin name="P1-14"/>
<pin name="P1-15"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P2-8"/>
<pin name="P2-9"/>
<pin name="P2-10"/>
<pin name="P2-11"/>
<pin name="P2-12"/>
<pin name="P2-13"/>
<pin name="P2-14"/>
<pin name="P2-15"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P3-8"/>
<pin name="P3-9"/>
<pin name="P3-10"/>
<pin name="P3-11"/>
<pin name="P3-12"/>
<pin name="P3-13"/>
<pin name="P3-14"/>
<pin name="P3-15"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="!BUSACT" direction="in"/>
<pin name="EBC0" direction="in"/>
<pin name="EBC1" direction="in"/>
<pin name="!RSTIN" direction="in"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="!NMI" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
</symbol>
<symbol name="6_VCCVSS">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
</symbol>
<symbol name="C165">
<pin name="P0L-1"/>
<pin name="P0L-2"/>
<pin name="P0L-3"/>
<pin name="P0L-4"/>
<pin name="P0L-5"/>
<pin name="P0L-6"/>
<pin name="P0L-7"/>
<pin name="P0H-0"/>
<pin name="P0H-1"/>
<pin name="P0H-2"/>
<pin name="P0H-3"/>
<pin name="P0H-4"/>
<pin name="P0H-5"/>
<pin name="P0H-6"/>
<pin name="P0H-7"/>
<pin name="P0L-0"/>
<pin name="P5-13" direction="in"/>
<pin name="P5-14" direction="in"/>
<pin name="P5-15" direction="in"/>
<pin name="P6-0"/>
<pin name="P6-1"/>
<pin name="P6-2"/>
<pin name="P6-3"/>
<pin name="P6-4"/>
<pin name="P6-5"/>
<pin name="P6-6"/>
<pin name="P1L-0"/>
<pin name="P1L-1"/>
<pin name="P1L-2"/>
<pin name="P1L-3"/>
<pin name="P1L-4"/>
<pin name="P1L-5"/>
<pin name="P1L-6"/>
<pin name="P1L-7"/>
<pin name="P1H-0"/>
<pin name="P1H-1"/>
<pin name="P1H-2"/>
<pin name="P1H-3"/>
<pin name="P1H-4"/>
<pin name="P1H-5"/>
<pin name="P1H-6"/>
<pin name="P1H-7"/>
<pin name="P2-8"/>
<pin name="P2-9"/>
<pin name="P2-10"/>
<pin name="P2-11"/>
<pin name="P2-12"/>
<pin name="P2-14"/>
<pin name="P2-15"/>
<pin name="P2-13"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P3-8"/>
<pin name="P3-9"/>
<pin name="P3-10"/>
<pin name="P3-11"/>
<pin name="P3-12"/>
<pin name="P3-13"/>
<pin name="P3-15"/>
<pin name="P5-12" direction="in"/>
<pin name="P5-10" direction="in"/>
<pin name="P5-11" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="P6-7"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="!RSTIN" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="!READY" direction="in"/>
<pin name="!WR!/!WRL" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="!NMI" direction="in"/>
<pin name="VPP" direction="pas"/>
</symbol>
<symbol name="C167">
<pin name="P5-0" direction="in"/>
<pin name="P5-1" direction="in"/>
<pin name="P5-2" direction="in"/>
<pin name="P5-3" direction="in"/>
<pin name="P5-4" direction="in"/>
<pin name="P5-5" direction="in"/>
<pin name="P5-6" direction="in"/>
<pin name="P5-7" direction="in"/>
<pin name="P5-8" direction="in"/>
<pin name="P5-9" direction="in"/>
<pin name="P5-10" direction="in"/>
<pin name="P5-11" direction="in"/>
<pin name="P5-12" direction="in"/>
<pin name="P5-13" direction="in"/>
<pin name="P5-14" direction="in"/>
<pin name="P5-15" direction="in"/>
<pin name="P0L-0"/>
<pin name="P0L-1"/>
<pin name="P0L-2"/>
<pin name="P0L-3"/>
<pin name="P0L-4"/>
<pin name="P0L-5"/>
<pin name="P0L-6"/>
<pin name="P0L-7"/>
<pin name="P0H-0"/>
<pin name="P0H-1"/>
<pin name="P0H-2"/>
<pin name="P0H-3"/>
<pin name="P0H-4"/>
<pin name="P0H-5"/>
<pin name="P0H-6"/>
<pin name="P0H-7"/>
<pin name="P1L-0"/>
<pin name="P1L-1"/>
<pin name="P1L-2"/>
<pin name="P1L-3"/>
<pin name="P1L-4"/>
<pin name="P1L-5"/>
<pin name="P1L-6"/>
<pin name="P1L-7"/>
<pin name="P1H-0"/>
<pin name="P1H-1"/>
<pin name="P1H-2"/>
<pin name="P1H-3"/>
<pin name="P1H-4"/>
<pin name="P1H-5"/>
<pin name="P1H-6"/>
<pin name="P1H-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P2-8"/>
<pin name="P2-9"/>
<pin name="P2-10"/>
<pin name="P2-11"/>
<pin name="P2-12"/>
<pin name="P2-13"/>
<pin name="P2-14"/>
<pin name="P2-15"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P3-8"/>
<pin name="P3-9"/>
<pin name="P3-10"/>
<pin name="P3-11"/>
<pin name="P3-12"/>
<pin name="P3-13"/>
<pin name="P3-15"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P6-0"/>
<pin name="P6-1"/>
<pin name="P6-2"/>
<pin name="P6-3"/>
<pin name="P6-4"/>
<pin name="P6-5"/>
<pin name="P6-6"/>
<pin name="P6-7"/>
<pin name="P7-0"/>
<pin name="P7-1"/>
<pin name="P7-2"/>
<pin name="P7-3"/>
<pin name="P7-4"/>
<pin name="P7-5"/>
<pin name="P7-6"/>
<pin name="P7-7"/>
<pin name="P8-0"/>
<pin name="P8-1"/>
<pin name="P8-2"/>
<pin name="P8-3"/>
<pin name="P8-4"/>
<pin name="P8-5"/>
<pin name="P8-6"/>
<pin name="P8-7"/>
<pin name="!RD" direction="out"/>
<pin name="!WR!/!WRL" direction="out"/>
<pin name="!READY" direction="in"/>
<pin name="!EA" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="!RSTIN" direction="in"/>
<pin name="!NMI" direction="in"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="VPP" direction="pas"/>
</symbol>
<symbol name="10VCCVSS">
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="VCC@7" direction="pwr"/>
<pin name="VCC@8" direction="pwr"/>
<pin name="VCC@9" direction="pwr"/>
<pin name="VCC@10" direction="pwr"/>
</symbol>
<symbol name="80186">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="TMRIN0"/>
<pin name="TMRIN1"/>
<pin name="TMROUT0" direction="out"/>
<pin name="TMROUT1" direction="out"/>
<pin name="DRQ0" direction="in"/>
<pin name="DRQ1" direction="in"/>
<pin name="A16/S3" direction="out"/>
<pin name="A17/S4" direction="out"/>
<pin name="A18/S5" direction="out"/>
<pin name="A19/S6" direction="out"/>
<pin name="!RES" direction="in"/>
<pin name="!PCS0" direction="out"/>
<pin name="!PCS1" direction="out"/>
<pin name="!PCS2" direction="out"/>
<pin name="!PCS3" direction="out"/>
<pin name="!PCS4" direction="out"/>
<pin name="!PCS5!/A1" direction="out"/>
<pin name="!PCS6!/A2" direction="out"/>
<pin name="!LCS" direction="out"/>
<pin name="!UCS" direction="out"/>
<pin name="!MCS0" direction="out"/>
<pin name="!MCS1" direction="out"/>
<pin name="!MCS2" direction="out"/>
<pin name="!MCS3" direction="out"/>
<pin name="!DEN" direction="out"/>
<pin name="DT/!R" direction="out"/>
<pin name="INT0" direction="in"/>
<pin name="INT1" direction="in"/>
<pin name="INT2/INTA0"/>
<pin name="INT3/INTA1"/>
<pin name="NMI"/>
<pin name="!TEST"/>
<pin name="!LOCK" direction="out"/>
<pin name="SRDY" direction="in"/>
<pin name="HOLD" direction="in"/>
<pin name="HLDA" direction="out"/>
<pin name="!S0" direction="out"/>
<pin name="!S1" direction="out"/>
<pin name="!S2" direction="out"/>
<pin name="ARDY" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="RESET" direction="out"/>
<pin name="X1" direction="out"/>
<pin name="X2" direction="out"/>
<pin name="ALE/QS0" direction="out"/>
<pin name="!RD!/!QSMD" direction="out"/>
<pin name="!WR!/QS1" direction="out"/>
<pin name="!BHE!/S7" direction="out"/>
</symbol>
<symbol name="2VCC2GND">
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="C503">
<pin name="P1-0" direction="in"/>
<pin name="P1-1" direction="in"/>
<pin name="P1-2" direction="in"/>
<pin name="P1-3" direction="in"/>
<pin name="P1-4" direction="in"/>
<pin name="P1-5" direction="in"/>
<pin name="P1-6" direction="in"/>
<pin name="P1-7" direction="in"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-3"/>
<pin name="P3-2"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
</symbol>
<symbol name="1VCC2VSS">
<pin name="VCC" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="80C517-M">
<pin name="P7-0" direction="in"/>
<pin name="P7-1" direction="in"/>
<pin name="P7-2" direction="in"/>
<pin name="P7-3" direction="in"/>
<pin name="P7-4" direction="in"/>
<pin name="P7-5" direction="in"/>
<pin name="P7-6" direction="in"/>
<pin name="P7-7" direction="in"/>
<pin name="P1-0"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P1-1"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P5-0"/>
<pin name="P5-1"/>
<pin name="P5-2"/>
<pin name="P5-3"/>
<pin name="P5-4"/>
<pin name="P5-5"/>
<pin name="P5-6"/>
<pin name="P5-7"/>
<pin name="P6-0"/>
<pin name="P6-1"/>
<pin name="P6-2"/>
<pin name="P6-3"/>
<pin name="P6-4"/>
<pin name="P6-5"/>
<pin name="P6-6"/>
<pin name="P6-7"/>
<pin name="P8-0" direction="in"/>
<pin name="P8-1" direction="in"/>
<pin name="P8-2" direction="in"/>
<pin name="P8-3" direction="in"/>
<pin name="!PE!/SWD" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="OWE" direction="in"/>
<pin name="!RO" direction="out"/>
<pin name="NC@17" direction="nc"/>
<pin name="NC@16" direction="nc"/>
<pin name="NC@15" direction="nc"/>
<pin name="NC@14" direction="nc"/>
<pin name="NC@13" direction="nc"/>
<pin name="NC@12" direction="nc"/>
<pin name="NC@11" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@6" direction="nc"/>
</symbol>
<symbol name="2VCC2VSS">
<pin name="VCC@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="2VCC3VSS">
<pin name="VCC@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
</symbol>
<symbol name="80C517-N">
<pin name="P7-0" direction="in"/>
<pin name="P7-1" direction="in"/>
<pin name="P7-2" direction="in"/>
<pin name="P7-3" direction="in"/>
<pin name="P7-4" direction="in"/>
<pin name="P7-5" direction="in"/>
<pin name="P7-6" direction="in"/>
<pin name="P7-7" direction="in"/>
<pin name="P1-0"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P1-1"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P5-0"/>
<pin name="P5-1"/>
<pin name="P5-2"/>
<pin name="P5-3"/>
<pin name="P5-4"/>
<pin name="P5-5"/>
<pin name="P5-6"/>
<pin name="P5-7"/>
<pin name="P6-0"/>
<pin name="P6-1"/>
<pin name="P6-2"/>
<pin name="P6-3"/>
<pin name="P6-4"/>
<pin name="P6-5"/>
<pin name="P6-6"/>
<pin name="P6-7"/>
<pin name="P8-0" direction="in"/>
<pin name="P8-1" direction="in"/>
<pin name="P8-2" direction="in"/>
<pin name="P8-3" direction="in"/>
<pin name="!PE!/SWD" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="OWE" direction="in"/>
<pin name="!RO" direction="out"/>
</symbol>
<symbol name="80C517NA">
<pin name="P7-0" direction="in"/>
<pin name="P7-1" direction="in"/>
<pin name="P7-2" direction="in"/>
<pin name="P7-3" direction="in"/>
<pin name="P7-4" direction="in"/>
<pin name="P7-5" direction="in"/>
<pin name="P7-6" direction="in"/>
<pin name="P7-7" direction="in"/>
<pin name="P1-0"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P1-1"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P5-0"/>
<pin name="P5-1"/>
<pin name="P5-2"/>
<pin name="P5-3"/>
<pin name="P5-4"/>
<pin name="P5-5"/>
<pin name="P5-6"/>
<pin name="P5-7"/>
<pin name="P6-0"/>
<pin name="P6-1"/>
<pin name="P6-2"/>
<pin name="P6-3"/>
<pin name="P6-4"/>
<pin name="P6-5"/>
<pin name="P6-6"/>
<pin name="P6-7"/>
<pin name="P8-0" direction="in"/>
<pin name="P8-1" direction="in"/>
<pin name="P8-2" direction="in"/>
<pin name="P8-3" direction="in"/>
<pin name="!PE!/SWD" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="OWE" direction="in"/>
<pin name="!RO" direction="out"/>
<pin name="!HWPD" direction="in"/>
</symbol>
<symbol name="80C517MA">
<pin name="P7-0" direction="in"/>
<pin name="P7-1" direction="in"/>
<pin name="P7-2" direction="in"/>
<pin name="P7-3" direction="in"/>
<pin name="P7-4" direction="in"/>
<pin name="P7-5" direction="in"/>
<pin name="P7-6" direction="in"/>
<pin name="P7-7" direction="in"/>
<pin name="P1-0"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P1-1"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P5-0"/>
<pin name="P5-1"/>
<pin name="P5-2"/>
<pin name="P5-3"/>
<pin name="P5-4"/>
<pin name="P5-5"/>
<pin name="P5-6"/>
<pin name="P5-7"/>
<pin name="P6-0"/>
<pin name="P6-1"/>
<pin name="P6-2"/>
<pin name="P6-3"/>
<pin name="P6-4"/>
<pin name="P6-5"/>
<pin name="P6-6"/>
<pin name="P6-7"/>
<pin name="P8-0" direction="in"/>
<pin name="P8-1" direction="in"/>
<pin name="P8-2" direction="in"/>
<pin name="P8-3" direction="in"/>
<pin name="!PE!/SWD" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="OWE" direction="in"/>
<pin name="!RO" direction="out"/>
<pin name="!HWPD" direction="in"/>
<pin name="NC@16" direction="nc"/>
<pin name="NC@15" direction="nc"/>
<pin name="NC@14" direction="nc"/>
<pin name="NC@13" direction="nc"/>
<pin name="NC@12" direction="nc"/>
<pin name="NC@11" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@6" direction="nc"/>
</symbol>
<symbol name="80515-N">
<pin name="AN0" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AN3" direction="in"/>
<pin name="AN4" direction="in"/>
<pin name="AN5" direction="in"/>
<pin name="AN6" direction="in"/>
<pin name="AN7" direction="in"/>
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P1-0"/>
<pin name="P1-1"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P5-0"/>
<pin name="P5-1"/>
<pin name="P5-2"/>
<pin name="P5-3"/>
<pin name="P5-4"/>
<pin name="P5-5"/>
<pin name="P5-6"/>
<pin name="P5-7"/>
<pin name="VPD" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VAGND" direction="in"/>
<pin name="VAREF" direction="in"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="VBB" direction="pas"/>
<pin name="!EA" direction="in"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
</symbol>
<symbol name="VCCVSS">
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="80C515-A">
<pin name="P6-0" direction="in"/>
<pin name="P6-1" direction="in"/>
<pin name="P6-2" direction="in"/>
<pin name="P6-3" direction="in"/>
<pin name="P6-4" direction="in"/>
<pin name="P6-5" direction="in"/>
<pin name="P6-6" direction="in"/>
<pin name="P6-7" direction="in"/>
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P1-0"/>
<pin name="P1-1"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P5-0"/>
<pin name="P5-1"/>
<pin name="P5-2"/>
<pin name="P5-3"/>
<pin name="P5-4"/>
<pin name="P5-5"/>
<pin name="P5-6"/>
<pin name="P5-7"/>
<pin name="!PE!/SWD" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="VAGND" direction="in"/>
<pin name="VAREF" direction="in"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!HWPD" direction="pas"/>
<pin name="!EA" direction="in"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
</symbol>
<symbol name="C501-LN">
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P1-0"/>
<pin name="P1-1"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
</symbol>
<symbol name="C501-LP">
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P1-0"/>
<pin name="P1-1"/>
<pin name="P1-2"/>
<pin name="P1-3"/>
<pin name="P1-4"/>
<pin name="P1-5"/>
<pin name="P1-6"/>
<pin name="P1-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="RESET" direction="in"/>
</symbol>
<symbol name="C503-LN">
<pin name="P1-0" direction="in"/>
<pin name="P1-1" direction="in"/>
<pin name="P1-2" direction="in"/>
<pin name="P1-3" direction="in"/>
<pin name="P1-4" direction="in"/>
<pin name="P1-5" direction="in"/>
<pin name="P1-6" direction="in"/>
<pin name="P1-7" direction="in"/>
<pin name="P0-0"/>
<pin name="P0-1"/>
<pin name="P0-2"/>
<pin name="P0-3"/>
<pin name="P0-4"/>
<pin name="P0-5"/>
<pin name="P0-6"/>
<pin name="P0-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
<pin name="!PSEN" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="8085AH">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="X1" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="SID" direction="in"/>
<pin name="TRAP" direction="in"/>
<pin name="RST5-5" direction="in"/>
<pin name="RST6-5" direction="in"/>
<pin name="RST7-5" direction="in"/>
<pin name="INTR" direction="in"/>
<pin name="READY" direction="in"/>
<pin name="!RESETIN" direction="in"/>
<pin name="HOLD" direction="in"/>
<pin name="RESETOUT" direction="out"/>
<pin name="SOD" direction="out"/>
<pin name="!INTA" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="S0" direction="out"/>
<pin name="S1" direction="out"/>
<pin name="IO/!M" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!WR" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="CLK" direction="out"/>
<pin name="HLDA" direction="out"/>
</symbol>
<symbol name="8088">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="READY" direction="in"/>
<pin name="INTR" direction="in"/>
<pin name="!TEST" direction="in"/>
<pin name="NMI" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="MN/!MX" direction="in"/>
<pin name="IO/!M" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!INTA" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="DT/!R" direction="in"/>
<pin name="!DEN" direction="in"/>
<pin name="!SS0" direction="in"/>
<pin name="HOLD"/>
<pin name="HLDA"/>
</symbol>
<symbol name="1VCC2GND">
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="8088-N">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="nc"/>
<pin name="!RD" direction="out"/>
<pin name="READY" direction="in"/>
<pin name="INTR" direction="in"/>
<pin name="!TEST" direction="in"/>
<pin name="NMI" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="MN/!MX" direction="in"/>
<pin name="IO/!M" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!INTA" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="DT/!R" direction="in"/>
<pin name="!DEN" direction="in"/>
<pin name="!SS0" direction="in"/>
<pin name="HOLD"/>
<pin name="HLDA"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
</symbol>
<symbol name="80188">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16/S3" direction="out"/>
<pin name="A17/S4" direction="out"/>
<pin name="A18/S5" direction="out"/>
<pin name="A19/S6" direction="out"/>
<pin name="!MCS0" direction="out"/>
<pin name="!MCS1" direction="out"/>
<pin name="!MCS2" direction="out"/>
<pin name="!PCS0" direction="out"/>
<pin name="!PCS1" direction="out"/>
<pin name="!PCS2" direction="out"/>
<pin name="!PCS3" direction="out"/>
<pin name="!PCS4" direction="out"/>
<pin name="!PCS5!/A1" direction="out"/>
<pin name="!PCS6!/A2" direction="out"/>
<pin name="TMROUT0" direction="out"/>
<pin name="TMROUT1" direction="out"/>
<pin name="DRQ0" direction="in"/>
<pin name="DRQ1" direction="in"/>
<pin name="!RES" direction="in"/>
<pin name="TMRIN0" direction="in"/>
<pin name="TMRIN1" direction="in"/>
<pin name="!LCS" direction="out"/>
<pin name="!UCS" direction="out"/>
<pin name="!DEN" direction="out"/>
<pin name="DT/!R" direction="out"/>
<pin name="!LOCK" direction="out"/>
<pin name="CLKOUT" direction="out"/>
<pin name="!S0" direction="out"/>
<pin name="!S1" direction="out"/>
<pin name="!S2" direction="out"/>
<pin name="INT0" direction="in"/>
<pin name="INT1" direction="in"/>
<pin name="INT2"/>
<pin name="INT3"/>
<pin name="NMI" direction="in"/>
<pin name="!TEST" direction="in"/>
<pin name="HOLD" direction="in"/>
<pin name="HLDA" direction="out"/>
<pin name="SRDY" direction="out"/>
<pin name="ARDY" direction="out"/>
<pin name="X1" direction="out"/>
<pin name="X2" direction="out"/>
<pin name="RESET" direction="out"/>
<pin name="!RD!/!QSMD" direction="out"/>
<pin name="ALE/QS0" direction="out"/>
<pin name="!WR!/QS1" direction="out"/>
<pin name="S7" direction="out"/>
<pin name="!MCS3" direction="out"/>
</symbol>
<symbol name="8086">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="A16/S3" direction="out"/>
<pin name="A17/S4" direction="out"/>
<pin name="A18/S5" direction="out"/>
<pin name="A19/S6" direction="out"/>
<pin name="!S0" direction="out"/>
<pin name="!S1" direction="out"/>
<pin name="!S2" direction="out"/>
<pin name="READY" direction="in"/>
<pin name="INTR" direction="in"/>
<pin name="!TEST" direction="in"/>
<pin name="NMI" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="MN/!MX" direction="in"/>
<pin name="!BHE!/S7" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="!LOCK" direction="out"/>
<pin name="QS0" direction="out"/>
<pin name="QS1" direction="out"/>
<pin name="!RQ!/!GT0"/>
<pin name="!RQ!/!GT1"/>
</symbol>
<symbol name="80286">
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="!S0" direction="out"/>
<pin name="!S1" direction="out"/>
<pin name="HLDA" direction="out"/>
<pin name="!BHE" direction="out"/>
<pin name="!PEACK" direction="out"/>
<pin name="!READY" direction="in"/>
<pin name="COD/!INTA" direction="out"/>
<pin name="M/!IO" direction="out"/>
<pin name="!LOCK" direction="out"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!ERROR" direction="in"/>
<pin name="INTR" direction="in"/>
<pin name="NMI" direction="in"/>
<pin name="PEREQ" direction="in"/>
<pin name="CAP" direction="in"/>
<pin name="HOLD" direction="in"/>
<pin name="!BUSY" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
</symbol>
<symbol name="2VCC3GND">
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="8237-A">
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DREQ0" direction="in"/>
<pin name="DREQ1" direction="in"/>
<pin name="DREQ2" direction="in"/>
<pin name="DREQ3" direction="in"/>
<pin name="DACK0" direction="out"/>
<pin name="DACK1" direction="out"/>
<pin name="DACK2" direction="out"/>
<pin name="DACK3" direction="out"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="!IOR"/>
<pin name="!IOW"/>
<pin name="!MEMR" direction="out"/>
<pin name="!MEMW" direction="out"/>
<pin name="ADSTB" direction="out"/>
<pin name="AEN" direction="out"/>
<pin name="HRQ" direction="out"/>
<pin name="EOP"/>
<pin name="-" direction="in"/>
<pin name="READY" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="HLDA" direction="in"/>
<pin name="RESET" direction="in"/>
</symbol>
<symbol name="VCCGND">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="8237-B">
<pin name="DB0"/>
<pin name="DB1"/>
<pin name="DB2"/>
<pin name="DB3"/>
<pin name="DB4"/>
<pin name="DB5"/>
<pin name="DB6"/>
<pin name="DB7"/>
<pin name="DREQ0" direction="in"/>
<pin name="DREQ1" direction="in"/>
<pin name="DREQ2" direction="in"/>
<pin name="DREQ3" direction="in"/>
<pin name="DACK0" direction="out"/>
<pin name="DACK1" direction="out"/>
<pin name="DACK2" direction="out"/>
<pin name="DACK3" direction="out"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="!IOR"/>
<pin name="!IOW"/>
<pin name="!MEMR" direction="out"/>
<pin name="!MEMW" direction="out"/>
<pin name="ADSTB" direction="out"/>
<pin name="AEN" direction="out"/>
<pin name="HRQ" direction="out"/>
<pin name="EOP"/>
<pin name="MODE" direction="in"/>
<pin name="READY" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="HLDA" direction="in"/>
<pin name="RESET" direction="in"/>
</symbol>
<symbol name="82C59A-2">
<pin name="IR0" direction="in"/>
<pin name="IR1" direction="in"/>
<pin name="IR2" direction="in"/>
<pin name="IR3" direction="in"/>
<pin name="IR4" direction="in"/>
<pin name="IR5" direction="in"/>
<pin name="IR6" direction="in"/>
<pin name="IR7" direction="in"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="!CS" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!INTA" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="CAS0"/>
<pin name="CAS1"/>
<pin name="CAS2"/>
<pin name="!SP!/!EN"/>
<pin name="INT" direction="out"/>
</symbol>
<symbol name="8282-A">
<pin name="DO0" direction="out"/>
<pin name="DO1" direction="out"/>
<pin name="DO2" direction="out"/>
<pin name="DO3" direction="out"/>
<pin name="DO4" direction="out"/>
<pin name="DO5" direction="out"/>
<pin name="DO6" direction="out"/>
<pin name="DO7" direction="out"/>
<pin name="DI0" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="DI3" direction="in"/>
<pin name="DI4" direction="in"/>
<pin name="DI5" direction="in"/>
<pin name="DI6" direction="in"/>
<pin name="DI7" direction="in"/>
<pin name="STB" direction="in"/>
<pin name="!OE" direction="in"/>
</symbol>
<symbol name="8283-A">
<pin name="!DO0" direction="out"/>
<pin name="!DO1" direction="out"/>
<pin name="!DO2" direction="out"/>
<pin name="!DO3" direction="out"/>
<pin name="!DO4" direction="out"/>
<pin name="!DO5" direction="out"/>
<pin name="!DO6" direction="out"/>
<pin name="!DO7" direction="out"/>
<pin name="DI0" direction="in"/>
<pin name="DI1" direction="in"/>
<pin name="DI2" direction="in"/>
<pin name="DI3" direction="in"/>
<pin name="DI4" direction="in"/>
<pin name="DI5" direction="in"/>
<pin name="DI6" direction="in"/>
<pin name="DI7" direction="in"/>
<pin name="STB" direction="in"/>
<pin name="!OE" direction="in"/>
</symbol>
<symbol name="8284-B">
<pin name="!AEN1" direction="in"/>
<pin name="!AEN2" direction="in"/>
<pin name="RDY1" direction="in"/>
<pin name="RDY2" direction="in"/>
<pin name="!ASYNC" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="F/!C" direction="in"/>
<pin name="EFI" direction="in"/>
<pin name="!RES" direction="in"/>
<pin name="CSYNC" direction="in"/>
<pin name="READY" direction="out"/>
<pin name="CLK" direction="out"/>
<pin name="PCLK" direction="out"/>
<pin name="OSC" direction="out"/>
<pin name="RESET" direction="out"/>
<pin name="X1" direction="in"/>
</symbol>
<symbol name="8286-A">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="B0"/>
<pin name="B1"/>
<pin name="B2"/>
<pin name="B3"/>
<pin name="B4"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="T" direction="in"/>
<pin name="!OE" direction="in"/>
</symbol>
<symbol name="8287-A">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="!B0"/>
<pin name="!B1"/>
<pin name="!B2"/>
<pin name="!B3"/>
<pin name="!B4"/>
<pin name="!B5"/>
<pin name="!B6"/>
<pin name="!B7"/>
<pin name="T" direction="in"/>
<pin name="!OE" direction="in"/>
</symbol>
<symbol name="8288-A">
<pin name="!S0" direction="in"/>
<pin name="!S1" direction="in"/>
<pin name="!S2" direction="in"/>
<pin name="IOB" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!AEN" direction="in"/>
<pin name="CEN" direction="in"/>
<pin name="DT/!R" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!MRDC" direction="out"/>
<pin name="!AMWC" direction="out"/>
<pin name="!MWTC" direction="out"/>
<pin name="!IOWC" direction="out"/>
<pin name="!IORC" direction="out"/>
<pin name="!INTA" direction="out"/>
<pin name="DEN" direction="out"/>
<pin name="MCE/!PDEN" direction="out"/>
<pin name="!AIOWC" direction="out"/>
</symbol>
<symbol name="8289">
<pin name="!S0" direction="in"/>
<pin name="!S1" direction="in"/>
<pin name="!S2" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!LOCK" direction="in"/>
<pin name="!CRQLCK" direction="in"/>
<pin name="RESB" direction="in"/>
<pin name="ANYRQST" direction="in"/>
<pin name="!IOB" direction="in"/>
<pin name="SYSB/!RESB" direction="in"/>
<pin name="!INIT" direction="in"/>
<pin name="!BCLK" direction="in"/>
<pin name="!BPRN" direction="in"/>
<pin name="!AEN" direction="out"/>
<pin name="!BREQ" direction="out"/>
<pin name="!BPRO" direction="out"/>
<pin name="!BUSY"/>
<pin name="!CBRQ"/>
</symbol>
<symbol name="82200">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="REQ0" direction="in"/>
<pin name="REQ1" direction="in"/>
<pin name="REQ2" direction="in"/>
<pin name="PACK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="INT/!DMA" direction="in"/>
<pin name="ACK0" direction="out"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="ACK1" direction="out"/>
<pin name="ACK2" direction="out"/>
<pin name="FREQ" direction="out"/>
<pin name="D3"/>
</symbol>
<symbol name="82C206">
<pin name="IRQ1" direction="in"/>
<pin name="IRQ3" direction="in"/>
<pin name="IRQ4" direction="in"/>
<pin name="IRQ5" direction="in"/>
<pin name="IRQ6" direction="in"/>
<pin name="IRQ7" direction="in"/>
<pin name="IRQ9" direction="in"/>
<pin name="IRQ10" direction="in"/>
<pin name="IRQ11" direction="in"/>
<pin name="IRQ12" direction="in"/>
<pin name="IRQ13" direction="in"/>
<pin name="IRQ14" direction="in"/>
<pin name="IRQ15" direction="in"/>
<pin name="XA9" direction="in"/>
<pin name="XA0"/>
<pin name="XA1"/>
<pin name="XA2"/>
<pin name="XA3"/>
<pin name="XA4"/>
<pin name="XA5"/>
<pin name="XA6"/>
<pin name="XA7"/>
<pin name="XA8"/>
<pin name="XD0"/>
<pin name="XD1"/>
<pin name="XD2"/>
<pin name="XD3"/>
<pin name="XD4"/>
<pin name="XD5"/>
<pin name="XD6"/>
<pin name="XD7"/>
<pin name="DREQ0" direction="in"/>
<pin name="DREQ1" direction="in"/>
<pin name="DREQ2" direction="in"/>
<pin name="DREQ3" direction="in"/>
<pin name="DREQ5" direction="in"/>
<pin name="DREQ6" direction="in"/>
<pin name="DREQ7" direction="in"/>
<pin name="DACK0" direction="out"/>
<pin name="DACK1" direction="out"/>
<pin name="DACK2" direction="out"/>
<pin name="DACK3" direction="out"/>
<pin name="DACK5" direction="out"/>
<pin name="DACK6" direction="out"/>
<pin name="DACK7" direction="out"/>
<pin name="XA16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
<pin name="PWRGD" direction="in"/>
<pin name="!PSRSTB" direction="in"/>
<pin name="!INTA" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="GATE2" direction="in"/>
<pin name="TMRCLK" direction="in"/>
<pin name="!ACK" direction="in"/>
<pin name="AS" direction="in"/>
<pin name="OSCI" direction="in"/>
<pin name="HLDA" direction="in"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
<pin name="!DMAMEMR" direction="out"/>
<pin name="!DMAMEMW" direction="out"/>
<pin name="!AEN8" direction="out"/>
<pin name="!AEN16" direction="out"/>
<pin name="ADSTB8" direction="out"/>
<pin name="ADSTB16" direction="out"/>
<pin name="TC" direction="out"/>
<pin name="HRQ" direction="out"/>
<pin name="INTR" direction="out"/>
<pin name="!XIOW"/>
<pin name="!XIOR"/>
<pin name="IOCHRDY"/>
</symbol>
<symbol name="82220-1">
<pin name="DX0"/>
<pin name="DX1"/>
<pin name="DX2"/>
<pin name="DX3"/>
<pin name="DX4"/>
<pin name="DX5"/>
<pin name="DX6"/>
<pin name="DX7"/>
<pin name="DX8"/>
<pin name="DX9"/>
<pin name="DX10"/>
<pin name="DX11"/>
<pin name="DX12"/>
<pin name="DX13"/>
<pin name="DX14"/>
<pin name="DX15"/>
<pin name="PX0/DX16"/>
<pin name="PX1/DX17"/>
<pin name="STBX" direction="in"/>
<pin name="!PEX" direction="in"/>
<pin name="SWAP" direction="in"/>
<pin name="INVY" direction="in"/>
<pin name="!DEN" direction="in"/>
<pin name="DIR0" direction="in"/>
<pin name="DIR1" direction="in"/>
<pin name="DIR2" direction="in"/>
<pin name="DY0"/>
<pin name="DY1"/>
<pin name="DY2"/>
<pin name="DY3"/>
<pin name="DY4"/>
<pin name="DY5"/>
<pin name="DY6"/>
<pin name="DY7"/>
<pin name="DY8"/>
<pin name="DY9"/>
<pin name="DY10"/>
<pin name="DY11"/>
<pin name="DY12"/>
<pin name="DY13"/>
<pin name="DY14"/>
<pin name="DY15"/>
<pin name="DY16/PY0"/>
<pin name="DY17/PY1"/>
<pin name="STBYZ" direction="in"/>
<pin name="DZ0"/>
<pin name="DZ1"/>
<pin name="DZ2"/>
<pin name="DZ3"/>
<pin name="DZ4"/>
<pin name="DZ5"/>
<pin name="DZ6"/>
<pin name="DZ7"/>
<pin name="DZ8"/>
<pin name="DZ9"/>
<pin name="DZ10"/>
<pin name="DZ11"/>
<pin name="DZ12"/>
<pin name="DZ13"/>
<pin name="DZ14"/>
<pin name="DZ15"/>
<pin name="DZ16/PZ0"/>
<pin name="DZ17/PZ1"/>
<pin name="BMOD" direction="in"/>
</symbol>
<symbol name="82220-2">
<pin name="DV0"/>
<pin name="DV1"/>
<pin name="DV2"/>
<pin name="DV3"/>
<pin name="DV4"/>
<pin name="DV5"/>
<pin name="DV6"/>
<pin name="DV7"/>
<pin name="DV8"/>
<pin name="DV9"/>
<pin name="DV10"/>
<pin name="DV11"/>
<pin name="DV12"/>
<pin name="DV13"/>
<pin name="DV14"/>
<pin name="DV15"/>
<pin name="DV24"/>
<pin name="DV25"/>
<pin name="STBV" direction="in"/>
<pin name="!PEV" direction="in"/>
<pin name="SWAP" direction="in"/>
<pin name="INVW" direction="in"/>
<pin name="!DEN" direction="in"/>
<pin name="DT/!R" direction="in"/>
<pin name="SUBMOD1" direction="in"/>
<pin name="SUBMOD0" direction="in"/>
<pin name="DW0"/>
<pin name="DW1"/>
<pin name="DW2"/>
<pin name="DW3"/>
<pin name="DW4"/>
<pin name="DW5"/>
<pin name="DW6"/>
<pin name="DW7"/>
<pin name="DW8"/>
<pin name="DW9"/>
<pin name="DW10"/>
<pin name="DW11"/>
<pin name="DW12"/>
<pin name="DW13"/>
<pin name="DW14"/>
<pin name="DW15"/>
<pin name="DW24"/>
<pin name="DW25"/>
<pin name="STBW" direction="in"/>
<pin name="DV16"/>
<pin name="DV17"/>
<pin name="DV18"/>
<pin name="DV19"/>
<pin name="DV20"/>
<pin name="DV21"/>
<pin name="DV22"/>
<pin name="DV23"/>
<pin name="DW16"/>
<pin name="DW17"/>
<pin name="DW18"/>
<pin name="DW19"/>
<pin name="DW20"/>
<pin name="DW21"/>
<pin name="DW22"/>
<pin name="DW23"/>
<pin name="DV26"/>
<pin name="DW26"/>
<pin name="BMOD" direction="in"/>
</symbol>
<symbol name="82220-3">
<pin name="DV0"/>
<pin name="DV1"/>
<pin name="DV2"/>
<pin name="DV3"/>
<pin name="DV4"/>
<pin name="DV5"/>
<pin name="DV6"/>
<pin name="DV7"/>
<pin name="DV8"/>
<pin name="DV9"/>
<pin name="DV10"/>
<pin name="DV11"/>
<pin name="DV12"/>
<pin name="DV13"/>
<pin name="DV14"/>
<pin name="DV15"/>
<pin name="!CS0" direction="out"/>
<pin name="!CS1" direction="out"/>
<pin name="STB" direction="in"/>
<pin name="CSMOD0" direction="in"/>
<pin name="CSMOD1" direction="in"/>
<pin name="INVW" direction="in"/>
<pin name="!DEN" direction="in"/>
<pin name="DT/!R" direction="in"/>
<pin name="SUBMOD1" direction="in"/>
<pin name="SUBMOD0" direction="in"/>
<pin name="DW0"/>
<pin name="DW1"/>
<pin name="DW2"/>
<pin name="DW3"/>
<pin name="DW4"/>
<pin name="DW5"/>
<pin name="DW6"/>
<pin name="DW7"/>
<pin name="DW8"/>
<pin name="DW9"/>
<pin name="DW10"/>
<pin name="DW11"/>
<pin name="DW12"/>
<pin name="DW13"/>
<pin name="DW14"/>
<pin name="DW15"/>
<pin name="!CS2" direction="out"/>
<pin name="!CS3" direction="out"/>
<pin name="CSMOD2" direction="in"/>
<pin name="DV16"/>
<pin name="DV17"/>
<pin name="DV18"/>
<pin name="DV19"/>
<pin name="DV20"/>
<pin name="DV21"/>
<pin name="DV22"/>
<pin name="DV23"/>
<pin name="DW16"/>
<pin name="DW17"/>
<pin name="DW18"/>
<pin name="DW19"/>
<pin name="DW20"/>
<pin name="DW21"/>
<pin name="DW22"/>
<pin name="DW23"/>
<pin name="!CCS" direction="in"/>
<pin name="!ENCS" direction="in"/>
<pin name="BMOD" direction="in"/>
</symbol>
<symbol name="82220-4">
<pin name="DV0"/>
<pin name="DV1"/>
<pin name="DV2"/>
<pin name="DV3"/>
<pin name="DV4"/>
<pin name="DV5"/>
<pin name="DV6"/>
<pin name="DV7"/>
<pin name="DV8"/>
<pin name="DV9"/>
<pin name="DV10"/>
<pin name="DV11"/>
<pin name="DV12"/>
<pin name="DV13"/>
<pin name="DV14"/>
<pin name="DV15"/>
<pin name="MOD286" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="STB" direction="in"/>
<pin name="DW16"/>
<pin name="DW17"/>
<pin name="INVW" direction="in"/>
<pin name="!DENIN" direction="in"/>
<pin name="DT/!RIN" direction="in"/>
<pin name="SUBMOD1" direction="in"/>
<pin name="SUBMOD0" direction="in"/>
<pin name="DW0"/>
<pin name="DW1"/>
<pin name="DW2"/>
<pin name="DW3"/>
<pin name="DW4"/>
<pin name="DW5"/>
<pin name="DW6"/>
<pin name="DW7"/>
<pin name="DW8"/>
<pin name="DW9"/>
<pin name="DW10"/>
<pin name="DW11"/>
<pin name="DW12"/>
<pin name="DW13"/>
<pin name="DW14"/>
<pin name="DW15"/>
<pin name="!S0" direction="in"/>
<pin name="!S1" direction="in"/>
<pin name="MB" direction="in"/>
<pin name="!IOWC" direction="out"/>
<pin name="!INTA" direction="out"/>
<pin name="MCE" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="DT/!ROUT" direction="out"/>
<pin name="!DENOUT" direction="out"/>
<pin name="SWAP" direction="in"/>
<pin name="!PEV" direction="in"/>
<pin name="!IORC" direction="out"/>
<pin name="!MWTC" direction="out"/>
<pin name="!S2" direction="in"/>
<pin name="!READY" direction="in"/>
<pin name="CMDLY" direction="in"/>
<pin name="CENL" direction="in"/>
<pin name="!AEN" direction="in"/>
<pin name="!MRDC" direction="out"/>
<pin name="DV16"/>
<pin name="DV17"/>
<pin name="BMOD" direction="in"/>
</symbol>
<symbol name="82220-5">
<pin name="DV0"/>
<pin name="DV1"/>
<pin name="DV2"/>
<pin name="DV3"/>
<pin name="DV4"/>
<pin name="DV5"/>
<pin name="DV6"/>
<pin name="DV7"/>
<pin name="DV8"/>
<pin name="DV9"/>
<pin name="DV10"/>
<pin name="DV11"/>
<pin name="DV12"/>
<pin name="DV13"/>
<pin name="DV14"/>
<pin name="DV15"/>
<pin name="MODE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SYSB" direction="in"/>
<pin name="!CBRQ"/>
<pin name="!BUSY"/>
<pin name="INVW" direction="in"/>
<pin name="!BPRN" direction="in"/>
<pin name="DT/!RIN" direction="in"/>
<pin name="SUBMOD1" direction="in"/>
<pin name="SUBMOD0" direction="in"/>
<pin name="DW0"/>
<pin name="DW1"/>
<pin name="DW2"/>
<pin name="DW3"/>
<pin name="DW4"/>
<pin name="DW5"/>
<pin name="DW6"/>
<pin name="DW7"/>
<pin name="DW8"/>
<pin name="DW9"/>
<pin name="DW10"/>
<pin name="DW11"/>
<pin name="DW12"/>
<pin name="DW13"/>
<pin name="DW14"/>
<pin name="DW15"/>
<pin name="!S0" direction="in"/>
<pin name="!S1" direction="in"/>
<pin name="!INIT" direction="in"/>
<pin name="!IOWC" direction="out"/>
<pin name="!INTA" direction="out"/>
<pin name="MCE" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!LLOCK" direction="out"/>
<pin name="!AEN" direction="out"/>
<pin name="SWAP" direction="in"/>
<pin name="!CBQLCK" direction="in"/>
<pin name="!IORC" direction="out"/>
<pin name="!MWTC" direction="out"/>
<pin name="!DENIN" direction="in"/>
<pin name="!READY" direction="in"/>
<pin name="!BCLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="M/!IO" direction="in"/>
<pin name="!MRDC" direction="out"/>
<pin name="!BPRO" direction="out"/>
<pin name="!BREQ" direction="out"/>
<pin name="BMOD" direction="in"/>
</symbol>
<symbol name="82220-6">
<pin name="DX0"/>
<pin name="DX1"/>
<pin name="DX2"/>
<pin name="DX3"/>
<pin name="DX4"/>
<pin name="DX5"/>
<pin name="DX6"/>
<pin name="DX7"/>
<pin name="DX8"/>
<pin name="DX9"/>
<pin name="DX10"/>
<pin name="DX11"/>
<pin name="DX12"/>
<pin name="DX13"/>
<pin name="DX14"/>
<pin name="DX15"/>
<pin name="DX16" direction="in"/>
<pin name="DX17" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="!AEN" direction="in"/>
<pin name="!DEN" direction="in"/>
<pin name="BMOD" direction="in"/>
<pin name="!BHE" direction="in"/>
<pin name="DA0" direction="out"/>
<pin name="DA1" direction="out"/>
<pin name="DA2" direction="out"/>
<pin name="DA3" direction="out"/>
<pin name="DA4" direction="out"/>
<pin name="DA5" direction="out"/>
<pin name="DA6" direction="out"/>
<pin name="DA7" direction="out"/>
<pin name="DA8" direction="out"/>
<pin name="DA9" direction="out"/>
<pin name="DA10" direction="out"/>
<pin name="DA11" direction="out"/>
<pin name="DA12" direction="out"/>
<pin name="DA13" direction="out"/>
<pin name="DA14" direction="out"/>
<pin name="DA15" direction="out"/>
<pin name="DA16" direction="out"/>
<pin name="DA17" direction="out"/>
<pin name="DY0"/>
<pin name="DY1"/>
<pin name="DY2"/>
<pin name="DY3"/>
<pin name="DY4"/>
<pin name="DY5"/>
<pin name="DY6"/>
<pin name="DY7"/>
<pin name="DY8"/>
<pin name="DY9"/>
<pin name="DY10"/>
<pin name="DY11"/>
<pin name="DY12"/>
<pin name="DY13"/>
<pin name="DY14"/>
<pin name="DY15"/>
<pin name="!BHEN" direction="out"/>
<pin name="SUBMOD0" direction="in"/>
<pin name="SUBMOD1" direction="in"/>
<pin name="DT/!R" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="SWAPEN" direction="in"/>
<pin name="RESET" direction="in"/>
</symbol>
<symbol name="82257">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D10"/>
<pin name="D9"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="HLDA" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!READY" direction="in"/>
<pin name="DREQ0" direction="in"/>
<pin name="DREQ1" direction="in"/>
<pin name="DREQ2" direction="in"/>
<pin name="DREQ3" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="HOLD" direction="out"/>
<pin name="!DACK0" direction="out"/>
<pin name="!DACK1" direction="out"/>
<pin name="!DACK2" direction="out"/>
<pin name="!DACK3" direction="out"/>
<pin name="M/!IO" direction="out"/>
<pin name="!S1"/>
<pin name="!S0"/>
<pin name="!BHE"/>
<pin name="!EOD0"/>
<pin name="!EOD1"/>
<pin name="!EOD2"/>
<pin name="!EOD3"/>
</symbol>
<symbol name="82258">
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="!EOD0"/>
<pin name="!EOD1"/>
<pin name="!EOD2"/>
<pin name="!EOD3"/>
<pin name="DREQ0" direction="in"/>
<pin name="DREQ1" direction="in"/>
<pin name="DREQ2" direction="in"/>
<pin name="DREQ3" direction="in"/>
<pin name="!DACK0" direction="out"/>
<pin name="!DACK1" direction="out"/>
<pin name="!DACK2" direction="out"/>
<pin name="!DACK3" direction="out"/>
<pin name="HOLD" direction="out"/>
<pin name="M/!IO" direction="out"/>
<pin name="HLDA" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!RD" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="!READY" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="!BHE"/>
<pin name="!S0"/>
<pin name="!S1"/>
</symbol>
<symbol name="82284">
<pin name="!RES" direction="in"/>
<pin name="!ARDY" direction="in"/>
<pin name="!SRDY" direction="in"/>
<pin name="!SRDYEN" direction="in"/>
<pin name="EFI" direction="in"/>
<pin name="F/!C" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="!S0" direction="in"/>
<pin name="!S1" direction="in"/>
<pin name="!ARDYEN" direction="in"/>
<pin name="X2" direction="in"/>
<pin name="!READY" direction="out"/>
<pin name="CLK" direction="out"/>
<pin name="RESET" direction="out"/>
<pin name="PCLK" direction="out"/>
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="82288">
<pin name="!READY" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="MB" direction="in"/>
<pin name="CMDLY" direction="in"/>
<pin name="CENL" direction="in"/>
<pin name="!S0" direction="in"/>
<pin name="!S1" direction="in"/>
<pin name="MCE" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!MRDC" direction="out"/>
<pin name="!MWTC" direction="out"/>
<pin name="!IOWC" direction="out"/>
<pin name="!IORC" direction="out"/>
<pin name="!INTA" direction="out"/>
<pin name="CEN" direction="in"/>
<pin name="M/!IO" direction="in"/>
<pin name="DEN" direction="out"/>
<pin name="DT/!R" direction="out"/>
</symbol>
<symbol name="82289">
<pin name="M/!IO" direction="in"/>
<pin name="!S1" direction="in"/>
<pin name="!READY" direction="in"/>
<pin name="SYSB" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!BCLK" direction="in"/>
<pin name="!INIT" direction="in"/>
<pin name="!BPRN" direction="in"/>
<pin name="!ALWAYS" direction="in"/>
<pin name="!LOCK" direction="in"/>
<pin name="!S0" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="!BREQ" direction="out"/>
<pin name="!BPRO" direction="out"/>
<pin name="!LLOCK" direction="out"/>
<pin name="!AEN" direction="out"/>
<pin name="!BUSY"/>
<pin name="!CBRQ"/>
</symbol>
<symbol name="82532">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="ALE" direction="in"/>
<pin name="BHE" direction="in" function="dot"/>
<pin name="CDA" direction="in"/>
<pin name="CDB" direction="in"/>
<pin name="CS" direction="in" function="dot"/>
<pin name="CTSA" direction="in" function="dot"/>
<pin name="CTSB" direction="in" function="dot"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="DACKA" direction="in" function="dot"/>
<pin name="DACKB" direction="in" function="dot"/>
<pin name="DRRA" direction="out"/>
<pin name="DRRB" direction="out"/>
<pin name="DRTA" direction="out"/>
<pin name="DRTB" direction="out"/>
<pin name="DTACK" direction="out" function="dot"/>
<pin name="IE0"/>
<pin name="IE1" direction="in"/>
<pin name="INT" direction="out"/>
<pin name="INTA" direction="in" function="dot"/>
<pin name="P00"/>
<pin name="P01"/>
<pin name="P02"/>
<pin name="P03"/>
<pin name="P04"/>
<pin name="P05"/>
<pin name="P06"/>
<pin name="P07"/>
<pin name="RD" direction="in" function="dot"/>
<pin name="RESET" direction="in"/>
<pin name="RTSA" direction="out" function="dot"/>
<pin name="RTSB" direction="out" function="dot"/>
<pin name="RXCLKA" direction="in"/>
<pin name="RXCLKB" direction="in"/>
<pin name="RXDA"/>
<pin name="RXDB"/>
<pin name="TXCLKA"/>
<pin name="TXCLKB"/>
<pin name="TXDA"/>
<pin name="TXDB"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="WITH" direction="in"/>
<pin name="WR" direction="in" function="dot"/>
<pin name="XTAL1" direction="pas"/>
<pin name="XTAL2" direction="pas"/>
</symbol>
<symbol name="BTS711">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="ST1/2" direction="oc"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT1" direction="out"/>
<pin name="OUT2" direction="out"/>
</symbol>
<symbol name="+VBB">
<pin name="+VBB@1" direction="pwr"/>
<pin name="+VBB@2" direction="pwr"/>
<pin name="+VBB@3" direction="pwr"/>
<pin name="+VBB@4" direction="pwr"/>
<pin name="+VBB@5" direction="pwr"/>
<pin name="+VBB@6" direction="pwr"/>
<pin name="+VBB@7" direction="pwr"/>
<pin name="+VBB@8" direction="pwr"/>
</symbol>
<symbol name="80C535">
<pin name="EA" direction="in"/>
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.4"/>
<pin name="P5.5"/>
<pin name="P5.6"/>
<pin name="P5.7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out"/>
<pin name="VAREF"/>
<pin name="VAGND"/>
<pin name="P6.0" direction="in"/>
<pin name="P6.1" direction="in"/>
<pin name="P6.2" direction="in"/>
<pin name="P6.3" direction="in"/>
<pin name="P6.4" direction="in"/>
<pin name="P6.6" direction="in"/>
<pin name="P6.7" direction="in"/>
<pin name="P4.3"/>
<pin name="P6.5" direction="in"/>
<pin name="P2.0"/>
<pin name="P4.2"/>
<pin name="P4.1"/>
<pin name="P4.0"/>
<pin name="P2.1"/>
<pin name="P2.2"/>
<pin name="P2.3"/>
<pin name="P2.4"/>
<pin name="P2.5"/>
<pin name="P2.6"/>
<pin name="P2.7"/>
<pin name="INT3/P1.0"/>
<pin name="INT4/P1.1"/>
<pin name="INT5/P1.2"/>
<pin name="INT6/P1.3"/>
<pin name="INT2/P1.4"/>
<pin name="T2EX/P1.5"/>
<pin name="CLKOUTP1.6"/>
<pin name="T2/P1.7"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR"/>
<pin name="P3.7/RD"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="2VCC1GND">
<pin name="GND@1" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
</symbol>
<symbol name="DPC31">
<pin name="ALE" direction="out"/>
<pin name="XPSEN" direction="out" function="dot"/>
<pin name="XCSDATA" direction="out" function="dot"/>
<pin name="RESET" direction="in"/>
<pin name="RXD_RXS" direction="in"/>
<pin name="XCSCODE" direction="out" function="dot"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="CLKOUTX2" direction="out"/>
<pin name="CLKOUTX4" direction="out"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="NTEST1" direction="in"/>
<pin name="NTEST2" direction="in"/>
<pin name="TST1" direction="in"/>
<pin name="BOOT0" direction="in"/>
<pin name="BOOT1" direction="in"/>
<pin name="BUS0" direction="in"/>
<pin name="BUS1" direction="in"/>
<pin name="BUS2" direction="in"/>
<pin name="PE0/D0"/>
<pin name="PE1/D1"/>
<pin name="PE2/D2"/>
<pin name="PE3/D3"/>
<pin name="PE4/D4"/>
<pin name="PE5/D5"/>
<pin name="PE6/D6"/>
<pin name="PE7/D7"/>
<pin name="XPLLEN" direction="in"/>
<pin name="PF0/A0" direction="in"/>
<pin name="PF1/A1" direction="in"/>
<pin name="PF2/A2" direction="in"/>
<pin name="PF3/A3" direction="in"/>
<pin name="PF4/A4" direction="in"/>
<pin name="PF5/A5" direction="in"/>
<pin name="PF6/A6" direction="in"/>
<pin name="PF7/A7" direction="in"/>
<pin name="PG0/A8" direction="in"/>
<pin name="PG1/A9" direction="in"/>
<pin name="PG2/A10" direction="in"/>
<pin name="PG3/A11" direction="in"/>
<pin name="PG4/A12" direction="in"/>
<pin name="PG5/XINT" direction="out"/>
<pin name="PG6/XCS" direction="in"/>
<pin name="PG7/XWR" direction="in"/>
<pin name="PH0/XRD" direction="in"/>
<pin name="PH1/VDD" direction="in"/>
<pin name="PH2/XRDY" direction="out"/>
<pin name="XCTS_RXA" direction="in" function="dot"/>
<pin name="TXD_TXS" direction="out"/>
<pin name="RTS_TXE" direction="out"/>
<pin name="SSDI" direction="in"/>
<pin name="SSCLK" direction="out"/>
<pin name="SSDO" direction="out"/>
<pin name="PA0/AD0"/>
<pin name="PA1/AD1"/>
<pin name="PA2/AD2"/>
<pin name="PA3/AD3"/>
<pin name="PA4/AD4"/>
<pin name="PA5/AD5"/>
<pin name="PA6/AD6"/>
<pin name="PA7/AD7"/>
<pin name="PC0/A8" direction="out"/>
<pin name="PC1/A9" direction="out"/>
<pin name="PC2/A10" direction="out"/>
<pin name="PC3/A11" direction="out"/>
<pin name="PC4/A12" direction="out"/>
<pin name="PC5/A13" direction="out"/>
<pin name="PC6/A14" direction="out"/>
<pin name="PC7/A15" direction="out"/>
<pin name="PB0/P1.0/T2"/>
<pin name="PB1/P1.1/T2EX"/>
<pin name="PB2/P1.2/RES"/>
<pin name="PB3/P1.3/IRR"/>
<pin name="PB4/P1.4"/>
<pin name="PB5/P1.5"/>
<pin name="PB6/P1.6"/>
<pin name="PB7/P1.7"/>
<pin name="PD0/P3.0/RXD"/>
<pin name="PD1/P3.1/TXD"/>
<pin name="PD2/XINT0"/>
<pin name="PD3/P3.3/XINT1"/>
<pin name="PD4/P3.4/T0"/>
<pin name="PD5/P3.5/T1"/>
<pin name="PD6/XWR"/>
<pin name="PD7/XRD"/>
<pin name="DBX" direction="in"/>
</symbol>
<symbol name="DPC31-P">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
</symbol>
<symbol name="80C535-1">
<pin name="EA" direction="in"/>
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.4"/>
<pin name="P5.5"/>
<pin name="P5.6"/>
<pin name="P5.7"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="PE" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="PSEN" direction="out"/>
<pin name="VAREF"/>
<pin name="VAGND"/>
<pin name="P6.0" direction="in"/>
<pin name="P6.1" direction="in"/>
<pin name="P6.2" direction="in"/>
<pin name="P6.3" direction="in"/>
<pin name="P6.4" direction="in"/>
<pin name="P6.6" direction="in"/>
<pin name="P6.7" direction="in"/>
<pin name="P4.3"/>
<pin name="P6.5" direction="in"/>
<pin name="P2.0"/>
<pin name="P4.2"/>
<pin name="P4.1"/>
<pin name="P4.0"/>
<pin name="P2.1"/>
<pin name="P2.2"/>
<pin name="P2.3"/>
<pin name="P2.4"/>
<pin name="P2.5"/>
<pin name="P2.6"/>
<pin name="P2.7"/>
<pin name="INT3/P1.0"/>
<pin name="INT4/P1.1"/>
<pin name="INT5/P1.2"/>
<pin name="INT6/P1.3"/>
<pin name="INT2/P1.4"/>
<pin name="T2EX/P1.5"/>
<pin name="CLKOUTP1.6"/>
<pin name="T2/P1.7"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4/T0"/>
<pin name="P3.5/T1"/>
<pin name="P3.6/WR"/>
<pin name="P3.7/RD"/>
</symbol>
<symbol name="BTS428L2">
<pin name="IN" direction="in"/>
<pin name="ST" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VBB" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="BTS555">
<pin name="IN" direction="in"/>
<pin name="IS" direction="pas"/>
<pin name="VBB" direction="pas"/>
<pin name="OUT1" direction="pas"/>
<pin name="OUT2" direction="pas"/>
</symbol>
<symbol name="SABC161CS">
<pin name="!NMI" direction="in" function="dot"/>
<pin name="ALE" direction="out" function="dot"/>
<pin name="BHE/WRH/P3.12" direction="in"/>
<pin name="CANRXD0/P4.4/A20"/>
<pin name="CANRXD1/P4.3/A19"/>
<pin name="CANTXD0/P4.6/A22"/>
<pin name="CANTXD1/P4.5/A21"/>
<pin name="CAPIN/P3.2" direction="in"/>
<pin name="CC24IO/P1H.4/A12"/>
<pin name="CC25IO/P1H.5/A13"/>
<pin name="CC26IO/P1H.6/A14"/>
<pin name="CC27IO/P1H.7/A15"/>
<pin name="EA" direction="in" function="dot"/>
<pin name="FOUT/CLKOUT/P3.15" direction="in"/>
<pin name="MRST/P3.8" direction="in"/>
<pin name="MTSR/P3.9" direction="in"/>
<pin name="P0H.0/AD8"/>
<pin name="P0H.1/AD9"/>
<pin name="P0H.2/AD10"/>
<pin name="P0H.3/AD11"/>
<pin name="P0H.4/AD12"/>
<pin name="P0H.5/AD13"/>
<pin name="P0H.6/AD14"/>
<pin name="P0H.7/AD15"/>
<pin name="P0L.0/AD0"/>
<pin name="P0L.1/AD1"/>
<pin name="P0L.2/AD2"/>
<pin name="P0L.3/AD3"/>
<pin name="P0L.4/AD4"/>
<pin name="P0L.5/AD5"/>
<pin name="P0L.6/AD6"/>
<pin name="P0L.7/AD7"/>
<pin name="P1H.0/A8"/>
<pin name="P1H.1/A9"/>
<pin name="P1H.2/A10"/>
<pin name="P1H.3/A11"/>
<pin name="P1L.0/A0"/>
<pin name="P1L.1/A1"/>
<pin name="P1L.2/A2"/>
<pin name="P1L.3/A3"/>
<pin name="P1L.4/A4"/>
<pin name="P1L.5/A5"/>
<pin name="P1L.6/A6"/>
<pin name="P1L.7/A7"/>
<pin name="P2.8" direction="in"/>
<pin name="P2.9" direction="in"/>
<pin name="P2.10" direction="in"/>
<pin name="P2.11" direction="in"/>
<pin name="P2.12" direction="in"/>
<pin name="P2.13" direction="in"/>
<pin name="P2.14" direction="in"/>
<pin name="P2.15" direction="in"/>
<pin name="P4.0/A16"/>
<pin name="P4.1/A17"/>
<pin name="P4.2/A18"/>
<pin name="P4.7/A23"/>
<pin name="P5.0/AN0" direction="in"/>
<pin name="P5.1/AN1" direction="in"/>
<pin name="P5.2/AN2" direction="in"/>
<pin name="P5.3/AN3" direction="in"/>
<pin name="P5.4/AN4" direction="in"/>
<pin name="P5.5/AN5" direction="in"/>
<pin name="P5.6/AN6" direction="in"/>
<pin name="P5.7/AN7" direction="in"/>
<pin name="P5.12" direction="in"/>
<pin name="P5.13" direction="in"/>
<pin name="P5.14" direction="in"/>
<pin name="P5.15" direction="in"/>
<pin name="P6.0/CS0" direction="out" function="dot"/>
<pin name="P6.1/CS1" direction="out" function="dot"/>
<pin name="P6.2/CS2" direction="out" function="dot"/>
<pin name="P6.3/CS3" direction="out" function="dot"/>
<pin name="P6.4/CS4" direction="out" function="dot"/>
<pin name="P6.5/HOLD" direction="out" function="dot"/>
<pin name="P6.6/HLDA" direction="out" function="dot"/>
<pin name="P6.7/BREQ" direction="out" function="dot"/>
<pin name="P7.4/CC28IO"/>
<pin name="P7.5/CC29IO"/>
<pin name="P7.6/CC30IO"/>
<pin name="P7.7/CC31IO"/>
<pin name="P9.0/SDA0"/>
<pin name="P9.1/SCL0"/>
<pin name="P9.2/SDA1"/>
<pin name="P9.3/SCL1"/>
<pin name="P9.4/SDA2"/>
<pin name="P9.5"/>
<pin name="RD" direction="out" function="dot"/>
<pin name="READY" direction="out" function="dot"/>
<pin name="RSTIN" function="dot"/>
<pin name="RSTOUT" direction="out" function="dot"/>
<pin name="RXD0/P3.11" direction="in"/>
<pin name="RXD1/T6OUT/P3.1" direction="in"/>
<pin name="SCLK/P3.13" direction="in"/>
<pin name="T2IN/P3.7" direction="in"/>
<pin name="T3EUD/P3.4" direction="in"/>
<pin name="T3IN/P3.6" direction="in"/>
<pin name="T3OUT/P3.3" direction="in"/>
<pin name="T4IN/P3.5" direction="in"/>
<pin name="TXD0/P3.10" direction="in"/>
<pin name="TXD1/T0IN/P3.0" direction="in"/>
<pin name="WR/WRL" direction="out" function="dot"/>
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="XTAL3" function="clk"/>
<pin name="XTAL4" function="clk"/>
</symbol>
<symbol name="PWR">
<pin name="VDD@0" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
</symbol>
<symbol name="APWR">
<pin name="VAGND" direction="pwr"/>
<pin name="VAREF" direction="pwr"/>
</symbol>
<symbol name="VSS-1">
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="C165-1">
<pin name="P0L-1"/>
<pin name="P0L-2"/>
<pin name="P0L-3"/>
<pin name="P0L-4"/>
<pin name="P0L-5"/>
<pin name="P0L-6"/>
<pin name="P0L-7"/>
<pin name="P0H-0"/>
<pin name="P0H-1"/>
<pin name="P0H-2"/>
<pin name="P0H-3"/>
<pin name="P0H-4"/>
<pin name="P0H-5"/>
<pin name="P0H-6"/>
<pin name="P0H-7"/>
<pin name="P0L-0"/>
<pin name="P5-13" direction="in"/>
<pin name="P5-14" direction="in"/>
<pin name="P5-15" direction="in"/>
<pin name="P6-0"/>
<pin name="P6-1"/>
<pin name="P6-2"/>
<pin name="P6-3"/>
<pin name="P6-4"/>
<pin name="P6-5"/>
<pin name="P6-6"/>
<pin name="P1L-0"/>
<pin name="P1L-1"/>
<pin name="P1L-2"/>
<pin name="P1L-3"/>
<pin name="P1L-4"/>
<pin name="P1L-5"/>
<pin name="P1L-6"/>
<pin name="P1L-7"/>
<pin name="P1H-0"/>
<pin name="P1H-1"/>
<pin name="P1H-2"/>
<pin name="P1H-3"/>
<pin name="P1H-4"/>
<pin name="P1H-5"/>
<pin name="P1H-6"/>
<pin name="P1H-7"/>
<pin name="P2-8"/>
<pin name="P2-9"/>
<pin name="P2-10"/>
<pin name="P2-11"/>
<pin name="P2-12"/>
<pin name="P2-14"/>
<pin name="P2-15"/>
<pin name="P2-13"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P3-8"/>
<pin name="P3-9"/>
<pin name="P3-10"/>
<pin name="P3-11"/>
<pin name="P3-12"/>
<pin name="P3-13"/>
<pin name="P3-15"/>
<pin name="P5-12" direction="in"/>
<pin name="P5-10" direction="in"/>
<pin name="P5-11" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="!EA" direction="in"/>
<pin name="P6-7"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="!RSTIN" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="!READY" direction="in"/>
<pin name="!WR!/!WRL" direction="out"/>
<pin name="!RD" direction="out"/>
<pin name="!NMI" direction="in"/>
<pin name="VPP" direction="pas"/>
</symbol>
<symbol name="C167-1">
<pin name="P5-0" direction="in"/>
<pin name="P5-1" direction="in"/>
<pin name="P5-2" direction="in"/>
<pin name="P5-3" direction="in"/>
<pin name="P5-4" direction="in"/>
<pin name="P5-5" direction="in"/>
<pin name="P5-6" direction="in"/>
<pin name="P5-7" direction="in"/>
<pin name="P5-8" direction="in"/>
<pin name="P5-9" direction="in"/>
<pin name="P5-10" direction="in"/>
<pin name="P5-11" direction="in"/>
<pin name="P5-12" direction="in"/>
<pin name="P5-13" direction="in"/>
<pin name="P5-14" direction="in"/>
<pin name="P5-15" direction="in"/>
<pin name="P0L-0"/>
<pin name="P0L-1"/>
<pin name="P0L-2"/>
<pin name="P0L-3"/>
<pin name="P0L-4"/>
<pin name="P0L-5"/>
<pin name="P0L-6"/>
<pin name="P0L-7"/>
<pin name="P0H-0"/>
<pin name="P0H-1"/>
<pin name="P0H-2"/>
<pin name="P0H-3"/>
<pin name="P0H-4"/>
<pin name="P0H-5"/>
<pin name="P0H-6"/>
<pin name="P0H-7"/>
<pin name="P1L-0"/>
<pin name="P1L-1"/>
<pin name="P1L-2"/>
<pin name="P1L-3"/>
<pin name="P1L-4"/>
<pin name="P1L-5"/>
<pin name="P1L-6"/>
<pin name="P1L-7"/>
<pin name="P1H-0"/>
<pin name="P1H-1"/>
<pin name="P1H-2"/>
<pin name="P1H-3"/>
<pin name="P1H-4"/>
<pin name="P1H-5"/>
<pin name="P1H-6"/>
<pin name="P1H-7"/>
<pin name="P2-0"/>
<pin name="P2-1"/>
<pin name="P2-2"/>
<pin name="P2-3"/>
<pin name="P2-4"/>
<pin name="P2-5"/>
<pin name="P2-6"/>
<pin name="P2-7"/>
<pin name="P2-8"/>
<pin name="P2-9"/>
<pin name="P2-10"/>
<pin name="P2-11"/>
<pin name="P2-12"/>
<pin name="P2-13"/>
<pin name="P2-14"/>
<pin name="P2-15"/>
<pin name="P3-0"/>
<pin name="P3-1"/>
<pin name="P3-2"/>
<pin name="P3-3"/>
<pin name="P3-4"/>
<pin name="P3-5"/>
<pin name="P3-6"/>
<pin name="P3-7"/>
<pin name="P3-8"/>
<pin name="P3-9"/>
<pin name="P3-10"/>
<pin name="P3-11"/>
<pin name="P3-12"/>
<pin name="P3-13"/>
<pin name="P3-15"/>
<pin name="P4-0"/>
<pin name="P4-1"/>
<pin name="P4-2"/>
<pin name="P4-3"/>
<pin name="P4-4"/>
<pin name="P4-5"/>
<pin name="P4-6"/>
<pin name="P4-7"/>
<pin name="P6-0"/>
<pin name="P6-1"/>
<pin name="P6-2"/>
<pin name="P6-3"/>
<pin name="P6-4"/>
<pin name="P6-5"/>
<pin name="P6-6"/>
<pin name="P6-7"/>
<pin name="P7-0"/>
<pin name="P7-1"/>
<pin name="P7-2"/>
<pin name="P7-3"/>
<pin name="P7-4"/>
<pin name="P7-5"/>
<pin name="P7-6"/>
<pin name="P7-7"/>
<pin name="P8-0"/>
<pin name="P8-1"/>
<pin name="P8-2"/>
<pin name="P8-3"/>
<pin name="P8-4"/>
<pin name="P8-5"/>
<pin name="P8-6"/>
<pin name="P8-7"/>
<pin name="!RD" direction="out"/>
<pin name="!WR!/!WRL" direction="out"/>
<pin name="!READY" direction="in"/>
<pin name="!EA" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="!RSTIN" direction="in"/>
<pin name="!NMI" direction="in"/>
<pin name="!RSTOUT" direction="out"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="VPP" direction="pas"/>
</symbol>
<symbol name="C167-1-1">
<pin name="ALE" direction="out" function="dot"/>
<pin name="!EA" direction="in" function="dot"/>
<pin name="!NMI" direction="in" function="dot"/>
<pin name="P.0/AN0" direction="in"/>
<pin name="P0.0/AD0"/>
<pin name="P0.1/AD1"/>
<pin name="P0.2/AD2"/>
<pin name="P0.3/AD3"/>
<pin name="P0.4/AD4"/>
<pin name="P0.5/AD5"/>
<pin name="P0.6/AD6"/>
<pin name="P0.7/AD7"/>
<pin name="P0.8/AD8"/>
<pin name="P0.9/AD9"/>
<pin name="P0.10/AD10"/>
<pin name="P0.11/AD11"/>
<pin name="P0.12/AD12"/>
<pin name="P0.13/AD13"/>
<pin name="P0.14/AD14"/>
<pin name="P0.15/AD15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.4/CC24"/>
<pin name="P1.5"/>
<pin name="P1.5/CC25"/>
<pin name="P1.6"/>
<pin name="P1.6/CC26"/>
<pin name="P1.7"/>
<pin name="P1.7/CC27"/>
<pin name="P1.8"/>
<pin name="P1.9"/>
<pin name="P1.10"/>
<pin name="P1.11"/>
<pin name="P2.0/CC0IO"/>
<pin name="P2.1/CC1IO"/>
<pin name="P2.2/CC2IO"/>
<pin name="P2.3/CC3IO"/>
<pin name="P2.4/CC4IO"/>
<pin name="P2.5/CC5IO"/>
<pin name="P2.6/CC6IO"/>
<pin name="P2.7/CC7IO"/>
<pin name="P2.8/EX0IN"/>
<pin name="P2.9/EX1IN"/>
<pin name="P2.10/EX2I"/>
<pin name="P2.11/EX3I"/>
<pin name="P2.12/EX4I"/>
<pin name="P2.13/EX5I"/>
<pin name="P2.14/EX6I"/>
<pin name="P2.15/EX7I"/>
<pin name="P3.0/T0IN"/>
<pin name="P3.1/T6OUT"/>
<pin name="P3.2/CAPIN"/>
<pin name="P3.3/T3OUT"/>
<pin name="P3.4/T3EUD"/>
<pin name="P3.5/T4IN"/>
<pin name="P3.6/T3IN"/>
<pin name="P3.7/T2IN"/>
<pin name="P3.8/MRST"/>
<pin name="P3.9/MTSR"/>
<pin name="P3.10/TXD0"/>
<pin name="P3.11/RXD0"/>
<pin name="P3.12/BHE"/>
<pin name="P3.13/SCLK"/>
<pin name="P3.15/CLKO"/>
<pin name="P4.0/A16"/>
<pin name="P4.1/A17"/>
<pin name="P4.2/A18"/>
<pin name="P4.3/A19"/>
<pin name="P4.4/A20"/>
<pin name="P4.5/A21"/>
<pin name="P4.6/A22"/>
<pin name="P4.7/A23"/>
<pin name="P5.1/AN1" direction="in"/>
<pin name="P5.2/AN2" direction="in"/>
<pin name="P5.3/AN3" direction="in"/>
<pin name="P5.4/AN4" direction="in"/>
<pin name="P5.5/AN5" direction="in"/>
<pin name="P5.6/AN6" direction="in"/>
<pin name="P5.7/AN7" direction="in"/>
<pin name="P5.8/AN8" direction="in"/>
<pin name="P5.9/AN9" direction="in"/>
<pin name="P5.10/AN10" direction="in"/>
<pin name="P5.11/AN11" direction="in"/>
<pin name="P5.12/AN12" direction="in"/>
<pin name="P5.13/AN13" direction="in"/>
<pin name="P5.14/AN14" direction="in"/>
<pin name="P5.15/AN15" direction="in"/>
<pin name="P6.0/CS0" function="dot"/>
<pin name="P6.1/CS1" function="dot"/>
<pin name="P6.2/CS2" function="dot"/>
<pin name="P6.3/CS3" function="dot"/>
<pin name="P6.4/CS4" function="dot"/>
<pin name="P6.5/HOLD" function="dot"/>
<pin name="P6.6/HLDA" function="dot"/>
<pin name="P6.7/BREQ" function="dot"/>
<pin name="P7.0/POUT0"/>
<pin name="P7.1/POUT1"/>
<pin name="P7.2/POUT2"/>
<pin name="P7.3/POUT3"/>
<pin name="P7.4CC28IO"/>
<pin name="P7.5CC29IO"/>
<pin name="P7.6CC30IO"/>
<pin name="P7.7CC31IO"/>
<pin name="P8.0CC16IO"/>
<pin name="P8.1CC17IO"/>
<pin name="P8.2CC18IO"/>
<pin name="P8.3CC19IO"/>
<pin name="P8.4CC20IO"/>
<pin name="P8.5CC21IO"/>
<pin name="P8.6CC22IO"/>
<pin name="P8.7CC23IO"/>
<pin name="!RD" direction="out" function="dot"/>
<pin name="!READY" direction="in" function="dot"/>
<pin name="!RSTIN" direction="in" function="dot"/>
<pin name="!RSTOUT" direction="out" function="dot"/>
<pin name="VAGND" direction="pas"/>
<pin name="VAREF" direction="pas"/>
<pin name="VPP" direction="pas"/>
<pin name="!WR!/!WRL" direction="out" function="dot"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="out" function="clk"/>
</symbol>
<symbol name="10VCCVSS-1">
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="VCC@7" direction="pwr"/>
<pin name="VCC@8" direction="pwr"/>
<pin name="VCC@9" direction="pwr"/>
<pin name="VCC@10" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
</symbol>
<symbol name="XC167-POWER">
<pin name="VDDP" direction="pwr"/>
<pin name="VDDP@1" direction="pwr"/>
<pin name="VDDP@2" direction="pwr"/>
<pin name="VDDP@3" direction="pwr"/>
<pin name="VDDP@4" direction="pwr"/>
<pin name="VDDP@5" direction="pwr"/>
<pin name="VDDP@6" direction="pwr"/>
<pin name="VSSP" direction="pwr"/>
<pin name="VSSP@1" direction="pwr"/>
<pin name="VSSP@2" direction="pwr"/>
<pin name="VSSP@3" direction="pwr"/>
<pin name="VSSP@4" direction="pwr"/>
<pin name="VSSP@5" direction="pwr"/>
<pin name="VDDI" direction="pwr"/>
<pin name="VDDI@1" direction="pwr"/>
<pin name="VDDI@2" direction="pwr"/>
<pin name="VSSI" direction="pwr"/>
<pin name="VSSI@1" direction="pwr"/>
<pin name="VSSI@2" direction="pwr"/>
<pin name="VSSI@3" direction="out"/>
</symbol>
<symbol name="XC167-BUS">
<pin name="P1L.0-A0-CC60"/>
<pin name="P1L.1-A1-COUT60"/>
<pin name="P1L.2-A2-CC61"/>
<pin name="P1L.3-A3-COUT61"/>
<pin name="P1L.4-A4-CC62"/>
<pin name="P1L.5-A5-COUT62"/>
<pin name="P1L.6-A6-COUT63"/>
<pin name="P1L.7-A7-/CTRAP-CC22"/>
<pin name="P1H.0-A8-/C6P0-CC23-E*"/>
<pin name="P1H.1-A9-/C6P1-MRST1"/>
<pin name="P1H.2-A10-/C6P2-MTSR1"/>
<pin name="P1H.3-A11-SCLK1-E*"/>
<pin name="P1H.4-A12-CC24IO"/>
<pin name="P1H.5-A13-CC25IO"/>
<pin name="P1H.6-A14-CC26IO"/>
<pin name="P1H.7-A15-CC27IO"/>
<pin name="P3.12-/BHE-/WRH"/>
<pin name="P4.0-A16"/>
<pin name="P4.1-A17"/>
<pin name="P4.2-A18"/>
<pin name="P4.3-A19"/>
<pin name="P4.4-A20-C*"/>
<pin name="P4.5-A21-C*"/>
<pin name="P4.6-A22-C*"/>
<pin name="P4.7-A23-C*"/>
<pin name="P6.0-/CS0-CC0IO"/>
<pin name="P6.1-/CS1-CC1IO"/>
<pin name="P6.2-/CS2-CC2IO"/>
<pin name="P6.3-/CS3-CC3IO"/>
<pin name="P6.4-/CS4-CC4IO"/>
<pin name="P6.5-/HOLD-CC5IO"/>
<pin name="P6.6-/HLDA-CC6IO"/>
<pin name="P6.7-/BREQ-CC7IO"/>
<pin name="P20.0-/RD"/>
<pin name="P20.1-/WR-/WRL"/>
<pin name="P20.2-READY"/>
<pin name="P20.5-/EA"/>
<pin name="P20.4-ALE"/>
<pin name="/RSTIN" direction="in"/>
<pin name="/NMI" direction="in"/>
<pin name="P20.12-/RSTOUT"/>
<pin name="P0L.0-AD0"/>
<pin name="P0L.1-AD1"/>
<pin name="P0L.2-AD2"/>
<pin name="P0L.3-AD3"/>
<pin name="P0L.4-AD4"/>
<pin name="P0L.5-AD5"/>
<pin name="P0L.6-AD6"/>
<pin name="P0L.7-AD7"/>
<pin name="P0H.0-AD8"/>
<pin name="P0H.1-AD9"/>
<pin name="P0H.2-AD10"/>
<pin name="P0H.3-AD11"/>
<pin name="P0H.4-AD12"/>
<pin name="P0H.5-AD13"/>
<pin name="P0H.6-AD14"/>
<pin name="P0H.7-AD15"/>
</symbol>
<symbol name="XC167-CLOCK-JTAG">
<pin name="P3.15-CLKOUT-F"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL3" direction="in"/>
<pin name="XTAL4" direction="out"/>
<pin name="/TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS-E*" direction="in"/>
<pin name="/BRKIN" direction="in"/>
<pin name="/BRKOUT" direction="out"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="XC167-PORTS">
<pin name="P2.8-CC8IO-EX0IN"/>
<pin name="P2.9-CC9IO-EX1IN"/>
<pin name="P2.10-CC10IO-EX2IN"/>
<pin name="P2.11-CC11IO-EX3IN"/>
<pin name="P2.12-CC12IO-EX4IN"/>
<pin name="P2.13-CC13IO-EX5IN"/>
<pin name="P2.14-CC14IO-EX6IN"/>
<pin name="P2.15-CC15IO-EX7IN-T7IN"/>
<pin name="P3.0-T0IN-TXD1-E*"/>
<pin name="P3.6-T3IN"/>
<pin name="P3.8-MRST0"/>
<pin name="P3.9-MTSR0"/>
<pin name="P3.10-TXD0-E*"/>
<pin name="P3.11-RXD0-E*"/>
<pin name="P3.13-SCLK0-E*"/>
<pin name="VAREF" direction="pas"/>
<pin name="VAGND" direction="pas"/>
<pin name="P5.0-AN0" direction="in"/>
<pin name="P5.1-AN1" direction="in"/>
<pin name="P5.2-AN2" direction="in"/>
<pin name="P5.3-AN3" direction="in"/>
<pin name="P5.4-AN4" direction="in"/>
<pin name="P5.5-AN5" direction="in"/>
<pin name="P5.6-AN6" direction="in"/>
<pin name="P5.7-AN7" direction="in"/>
<pin name="P5.12-AN12-T6IN" direction="in"/>
<pin name="P5.13-AN13-T5IN" direction="in"/>
<pin name="P5.14-AN14-T4EUD" direction="in"/>
<pin name="P5.15-AN15-T2EUD" direction="in"/>
<pin name="P7.4-CC28IO-C*"/>
<pin name="P7.5-CC29IO-C*"/>
<pin name="P7.6-CC30IO-C*"/>
<pin name="P7.7-CC31IO-C*"/>
<pin name="P9.0-SDA0-CC16IO-C*"/>
<pin name="P9.1-SCL0-CC17IO-C*"/>
<pin name="P9.2-SDA1-CC18IO-C*"/>
<pin name="P9.3-SCL1-CC19IO-C*"/>
<pin name="P9.4-SDA2-CC20IO"/>
<pin name="P9.5-SCL2-CC21IO"/>
<pin name="P5.8-AN8" direction="in"/>
<pin name="P5.9-AN9" direction="in"/>
<pin name="P5.10-AN10-T6EUD" direction="in"/>
<pin name="P5.11-AN11-T5EUD" direction="in"/>
<pin name="P3.1-T6OUT-RXD1-E*"/>
<pin name="P3.2-CAPIN"/>
<pin name="P3.3-T3OUT"/>
<pin name="P3.4-T3EUD"/>
<pin name="P3.5-T4IN"/>
<pin name="P3.7-T2IN"/>
</symbol>
<symbol name="XC167CI">
<pin name="/BRKIN" function="dot"/>
<pin name="/BRKOUT" function="dot"/>
<pin name="/EA-P20.5" function="dot"/>
<pin name="/NMI" function="dot"/>
<pin name="/RESET-IN" function="dot"/>
<pin name="/RESET-OUT" function="dot"/>
<pin name="/TRST" function="dot"/>
<pin name="NC@0"/>
<pin name="NC@1"/>
<pin name="NC@2"/>
<pin name="NC@3"/>
<pin name="NC@4"/>
<pin name="NC@5"/>
<pin name="P0H.0-AD8"/>
<pin name="P0H.1-AD9"/>
<pin name="P0H.2-AD10"/>
<pin name="P0H.3-AD11"/>
<pin name="P0H.4-AD12"/>
<pin name="P0H.5-AD13"/>
<pin name="P0H.6-AD14"/>
<pin name="P0H.7-AD15"/>
<pin name="P0L.0-AD0"/>
<pin name="P0L.1-AD1"/>
<pin name="P0L.2-AD2"/>
<pin name="P0L.3-AD3"/>
<pin name="P0L.4-AD4"/>
<pin name="P0L.5-AD5"/>
<pin name="P0L.6-AD6"/>
<pin name="P0L.7-AD7"/>
<pin name="P1H.0-A8"/>
<pin name="P1H.1-A9"/>
<pin name="P1H.2-A10"/>
<pin name="P1H.3-A11"/>
<pin name="P1H.4-A12"/>
<pin name="P1H.5-A13"/>
<pin name="P1H.6-A14"/>
<pin name="P1H.7-A15"/>
<pin name="P1L.0-A0"/>
<pin name="P1L.1-A1"/>
<pin name="P1L.2-A2"/>
<pin name="P1L.3-A3"/>
<pin name="P1L.4-A4"/>
<pin name="P1L.5-A5"/>
<pin name="P1L.6-A6"/>
<pin name="P1L.7-A7"/>
<pin name="P2.8-CC8IO-EX0IN"/>
<pin name="P2.9-CC9IO-EX1IN"/>
<pin name="P2.10-CC10IO-EX2IN"/>
<pin name="P2.11-CC11IO-EX3IN"/>
<pin name="P2.12-CC12IO-EX4IN"/>
<pin name="P2.13-CC13IO-EX5IN"/>
<pin name="P2.14-CC14IO-EX6IN"/>
<pin name="P2.15-CC15IO-EX7IN-T7IN"/>
<pin name="P3.0-T0IN-TXD1-E*"/>
<pin name="P3.1-T6OUT-RXD0-E*"/>
<pin name="P3.2-CAPIN"/>
<pin name="P3.3-T3OUT"/>
<pin name="P3.4-T3EUD"/>
<pin name="P3.5-T4IN"/>
<pin name="P3.6-T3IN"/>
<pin name="P3.7-T2IN"/>
<pin name="P3.8-MRST0"/>
<pin name="P3.9-MTSR0"/>
<pin name="P3.10-TXD0-E*"/>
<pin name="P3.11-RXD0-E*"/>
<pin name="P3.12-/BHE-/WRH"/>
<pin name="P3.13-SCLK0-E*"/>
<pin name="P3.15-CLKOUT-F"/>
<pin name="P4.0-A16"/>
<pin name="P4.1-A17"/>
<pin name="P4.2-A18"/>
<pin name="P4.3-A19"/>
<pin name="P4.4-A20-C*"/>
<pin name="P4.5-A21-C*"/>
<pin name="P4.6-A22-C*"/>
<pin name="P4.7-A23-C*"/>
<pin name="P5.0-AN0"/>
<pin name="P5.1-AN1"/>
<pin name="P5.2-AN2"/>
<pin name="P5.3-AN3"/>
<pin name="P5.4-AN4"/>
<pin name="P5.5-AN5"/>
<pin name="P5.6-AN6"/>
<pin name="P5.7-AN7"/>
<pin name="P5.8-AN8"/>
<pin name="P5.9-AN9"/>
<pin name="P5.10-AN10"/>
<pin name="P5.11-AN11"/>
<pin name="P5.12-AN12"/>
<pin name="P5.13-AN13"/>
<pin name="P5.14-AN14"/>
<pin name="P5.15-AN15"/>
<pin name="P6.0-/CS0-CC0IO"/>
<pin name="P6.1-/CS1-CC1IO"/>
<pin name="P6.2-/CS2-CC2IO"/>
<pin name="P6.3-/CS3-CC3IO"/>
<pin name="P6.4-/CS4-CC4IO"/>
<pin name="P6.5-/HOLD-CC5IO"/>
<pin name="P6.6-/HLDA-CC6IO"/>
<pin name="P6.7-/BREQ-CC7IO"/>
<pin name="P7.4-CC28IO-C*"/>
<pin name="P7.5-CC29IO-C*"/>
<pin name="P7.6-CC30IO-C*"/>
<pin name="P7.7-CC31IO-C*"/>
<pin name="P9.0-SDA0-CC16IO-C*"/>
<pin name="P9.1-SCL0-CC17IO-C*"/>
<pin name="P9.2-SDA1-CC18IO-C*"/>
<pin name="P9.3-SCL1-CC19IO-C*"/>
<pin name="P9.4-SDA2-CC20IO-C*"/>
<pin name="P9.5-SCL2-CC21IO-C*"/>
<pin name="P20.0-/RD"/>
<pin name="P20.1-/WR-/WRL"/>
<pin name="P20.2-READY"/>
<pin name="P20.4-ALE"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS-E"/>
<pin name="VAGND"/>
<pin name="VAREF"/>
<pin name="VDDI@0" direction="pwr"/>
<pin name="VDDI@1" direction="pwr"/>
<pin name="VDDI@2" direction="pwr"/>
<pin name="VDDP@0" direction="pwr"/>
<pin name="VDDP@1" direction="pwr"/>
<pin name="VDDP@3" direction="pwr"/>
<pin name="VDDP@4" direction="pwr"/>
<pin name="VDDP@5" direction="pwr"/>
<pin name="VDDP@6" direction="pwr"/>
<pin name="VDDP@7" direction="pwr"/>
<pin name="VSSI@0" direction="pwr"/>
<pin name="VSSI@1" direction="pwr"/>
<pin name="VSSI@2" direction="pwr"/>
<pin name="VSSI@3" direction="pwr"/>
<pin name="VSSP@0" direction="pwr"/>
<pin name="VSSP@1" direction="pwr"/>
<pin name="VSSP@2" direction="pwr"/>
<pin name="VSSP@4" direction="pwr"/>
<pin name="VSSP@5" direction="pwr"/>
<pin name="VSSP@6" direction="pwr"/>
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="XTAL3" function="clk"/>
<pin name="XTAL4" function="clk"/>
</symbol>
<symbol name="C167-2">
<pin name="ALE" direction="out" function="dot"/>
<pin name="!EA" direction="in" function="dot"/>
<pin name="!NMI" direction="in" function="dot"/>
<pin name="P.0/AN0" direction="in"/>
<pin name="P0.0/AD0"/>
<pin name="P0.1/AD1"/>
<pin name="P0.2/AD2"/>
<pin name="P0.3/AD3"/>
<pin name="P0.4/AD4"/>
<pin name="P0.5/AD5"/>
<pin name="P0.6/AD6"/>
<pin name="P0.7/AD7"/>
<pin name="P0.8/AD8"/>
<pin name="P0.9/AD9"/>
<pin name="P0.10/AD10"/>
<pin name="P0.11/AD11"/>
<pin name="P0.12/AD12"/>
<pin name="P0.13/AD13"/>
<pin name="P0.14/AD14"/>
<pin name="P0.15/AD15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.4/CC24"/>
<pin name="P1.5"/>
<pin name="P1.5/CC25"/>
<pin name="P1.6"/>
<pin name="P1.6/CC26"/>
<pin name="P1.7"/>
<pin name="P1.7/CC27"/>
<pin name="P1.8"/>
<pin name="P1.9"/>
<pin name="P1.10"/>
<pin name="P1.11"/>
<pin name="P2.0/CC0IO"/>
<pin name="P2.1/CC1IO"/>
<pin name="P2.2/CC2IO"/>
<pin name="P2.3/CC3IO"/>
<pin name="P2.4/CC4IO"/>
<pin name="P2.5/CC5IO"/>
<pin name="P2.6/CC6IO"/>
<pin name="P2.7/CC7IO"/>
<pin name="P2.8/EX0IN"/>
<pin name="P2.9/EX1IN"/>
<pin name="P2.10/EX2I"/>
<pin name="P2.11/EX3I"/>
<pin name="P2.12/EX4I"/>
<pin name="P2.13/EX5I"/>
<pin name="P2.14/EX6I"/>
<pin name="P2.15/EX7I"/>
<pin name="P3.0/T0IN"/>
<pin name="P3.1/T6OUT"/>
<pin name="P3.2/CAPIN"/>
<pin name="P3.3/T3OUT"/>
<pin name="P3.4/T3EUD"/>
<pin name="P3.5/T4IN"/>
<pin name="P3.6/T3IN"/>
<pin name="P3.7/T2IN"/>
<pin name="P3.8/MRST"/>
<pin name="P3.9/MTSR"/>
<pin name="P3.10/TXD0"/>
<pin name="P3.11/RXD0"/>
<pin name="P3.12/BHE"/>
<pin name="P3.13/SCLK"/>
<pin name="P3.15/CLKO"/>
<pin name="P4.0/A16"/>
<pin name="P4.1/A17"/>
<pin name="P4.2/A18"/>
<pin name="P4.3/A19"/>
<pin name="P4.4/A20"/>
<pin name="P4.5/A21"/>
<pin name="P4.6/A22"/>
<pin name="P4.7/A23"/>
<pin name="P5.1/AN1" direction="in"/>
<pin name="P5.2/AN2" direction="in"/>
<pin name="P5.3/AN3" direction="in"/>
<pin name="P5.4/AN4" direction="in"/>
<pin name="P5.5/AN5" direction="in"/>
<pin name="P5.6/AN6" direction="in"/>
<pin name="P5.7/AN7" direction="in"/>
<pin name="P5.8/AN8" direction="in"/>
<pin name="P5.9/AN9" direction="in"/>
<pin name="P5.10/AN10" direction="in"/>
<pin name="P5.11/AN11" direction="in"/>
<pin name="P5.12/AN12" direction="in"/>
<pin name="P5.13/AN13" direction="in"/>
<pin name="P5.14/AN14" direction="in"/>
<pin name="P5.15/AN15" direction="in"/>
<pin name="P6.0/!CS0" function="dot"/>
<pin name="P6.1/!CS1" function="dot"/>
<pin name="P6.2/!CS2" function="dot"/>
<pin name="P6.3/!CS3" function="dot"/>
<pin name="P6.4/!CS4" function="dot"/>
<pin name="P6.5/HOLD" function="dot"/>
<pin name="P6.6/HLDA" function="dot"/>
<pin name="P6.7/BREQ" function="dot"/>
<pin name="P7.0/POUT0"/>
<pin name="P7.1/POUT1"/>
<pin name="P7.2/POUT2"/>
<pin name="P7.3/POUT3"/>
<pin name="P7.4CC28IO"/>
<pin name="P7.5CC29IO"/>
<pin name="P7.6CC30IO"/>
<pin name="P7.7CC31IO"/>
<pin name="P8.0CC16IO"/>
<pin name="P8.1CC17IO"/>
<pin name="P8.2CC18IO"/>
<pin name="P8.3CC19IO"/>
<pin name="P8.4CC20IO"/>
<pin name="P8.5CC21IO"/>
<pin name="P8.6CC22IO"/>
<pin name="P8.7CC23IO"/>
<pin name="!RD" direction="out" function="dot"/>
<pin name="!READY" direction="in" function="dot"/>
<pin name="!RSTIN" direction="in" function="dot"/>
<pin name="!RSTOUT" direction="out" function="dot"/>
<pin name="VAGND" direction="pas"/>
<pin name="VAREF" direction="pas"/>
<pin name="VPP" direction="pas"/>
<pin name="!WR!/!WRL" direction="out" function="dot"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="out" function="clk"/>
</symbol>
<symbol name="SAK-XC226*">
<pin name="VSS@0" direction="pwr"/>
<pin name="VDDPB@0" direction="pwr"/>
<pin name="/TESTM" function="dot"/>
<pin name="TDI_C/P7,2/EMUX0/TXDC4/CCU62_CCPOS0A"/>
<pin name="/TRST" function="dot"/>
<pin name="TDO/P7.0/T3OUT/T6OUT/RXDC4B"/>
<pin name="TMS_C/P7.3/EMUX1/U01_DOUT/U0C0_DOUT/CCU62_CCPOS1A/U0C1DX0F"/>
<pin name="/BRKIN_C/P7.1/EXTCLK/TXDC4/CCU62_CTRAPA"/>
<pin name="TCK_C/P7.4/EMUX2/U0C1DOUT/U0C1_SCLK/CCU62_CCPOS2A/U0C0_DX0D/U1C1_DX1E"/>
<pin name="VDDIM@0"/>
<pin name="P6.0/EMUX0/U1C1_DOUT/!BRKOUT/ADCX_REQGTYC/U1C1_DX0E"/>
<pin name="P6.1/EMUX1/T3OUT/U1C1_DOUT/ADCX_REQTRYC"/>
<pin name="P6.2/EMUX2/T6OUT/U1C1_SCLK/U1C1_DXC1"/>
<pin name="VDDPA@0"/>
<pin name="P15.0/ADC1_CH0"/>
<pin name="P15.2/ADC1_CH2/T5IN"/>
<pin name="P15.4/ADC1_CH4/T6IN"/>
<pin name="P15.5/ADC1_CH5/T6EUD"/>
<pin name="P15.6/ADC1_CH6"/>
<pin name="VAREF"/>
<pin name="VAGND"/>
<pin name="P5.0/ADC0_CH0"/>
<pin name="TDI_A/P5.2/ADC0_CH2"/>
<pin name="P5.3/ADC0_CH3/T3IN"/>
<pin name="VDDPB@2"/>
<pin name="VSS@1"/>
<pin name="VDDPB@3"/>
<pin name="TMS_A/P5.4/ADC0_CH4/CCU63_T12HRB/T3EUD"/>
<pin name="P5.5/ADC0_CH5/CCU60_T12HRB"/>
<pin name="P5.8/ADC0_CH8/CCU6X_T12HRC/CCU6X_T13HRC"/>
<pin name="P5.9/ADC0_CH9/CC2_T7IN"/>
<pin name="/BRKIN_A/P5.10/ADC0_CH10"/>
<pin name="P5.11/ADC0_CH11"/>
<pin name="P5.13/ADC0_CH10/EX0BINB"/>
<pin name="P5.15/ADC0_CH15"/>
<pin name="P2.12/U0C0_SELO4/U0C1_SELO3/READY"/>
<pin name="P2.11/U0C0_SELO2/U0C1_SELO2/!BHE/!WRH"/>
<pin name="VDD@1"/>
<pin name="P2.0/CCU63_CC60/AD13/RXDC0C"/>
<pin name="P2.1/TXDC0/CCU63_CC61/AD14/EX0AINA"/>
<pin name="P2.2/TXDC1/CCU63_CC62/AD15/EX1AINA"/>
<pin name="P4.0/CC2_8/!CS0" function="dot"/>
<pin name="P2.3/U0C0_DOUT/CCU63_COUT63/CC2_0/A16/U0C0_DX0E/U0C1_DX0D/RXDC0A"/>
<pin name="P4.1/TXDC2/CC2_9/!CS1" function="dot"/>
<pin name="P2.4/U0C1_DOUT/TXDC0/CC2_1/A17/U0C0_DX0F/RXDC1A"/>
<pin name="P2.5/U0C0_SCLKOUT/TXDC0/CC2_2/A18/A0C0_DX1D"/>
<pin name="P4.2/TXDC2/CC2_10/T2IN/!CS2" function="dot"/>
<pin name="P2.6/U0C0_SELO0/U0C1_SELO1/CC2_3/A19/U0C0_DX2D/RXDC0D"/>
<pin name="P4.3/CC2_11/RXDC2A/T2EUD/!CS3" function="dot"/>
<pin name="VDDPB@4"/>
<pin name="VSS@2"/>
<pin name="VDDPB@5"/>
<pin name="P0.0/U1C0_DOUT/CCU61_CC60/U1C0_DX0A/A0"/>
<pin name="P2.7/U0C1_SELO0/U0C0_SELO1/CC2_4/A20/U0C1_DX2C/RXDC1C"/>
<pin name="P0.1/U1C0_DOUT/TXDC0/CCU61_CC61/U1C0_DX0B/U1C0_DX1A/A1"/>
<pin name="P2.8/U0C1_SCLKOUT/EXTCLK/CC2_5/A21/U0C1_DX1D"/>
<pin name="TCK_A/P2.9/U0C1_DOUT/TXDC1/CC2_6/A22/DIRIN/"/>
<pin name="P0.2/U1C0_SCLKOUT/TXDC0/CCU61_CC62/U1C0_DX1B/A2"/>
<pin name="P10.0/U0C1_DOUT/CCU60_CC60/U0C0_DX0A/U0C1DX0A/AD0"/>
<pin name="P10.1/U0C0_DOUT/CCU60_CC61/U0C0_DX0B/U0C0_DX1A/AD1"/>
<pin name="P0.3/U1C0_SELO0/U1C1/SELO1/CCU61_COUT60/U1C0_DX2A/DXDC0B/A3"/>
<pin name="P10.2/U0C0_SCLKOUT/U0C0_DX1B/AD2"/>
<pin name="P0.4/U1C1_SELO0/U1C0_SELO1/CCU61_COUT61/U1C1_DX2A/RXDC1B/A4"/>
<pin name="VDDI@1"/>
<pin name="TREF"/>
<pin name="P2.10/U0C1_DOUT/U0C0_SELO3/CC2_7/A23/U0C1_DX0E/CAPIN"/>
<pin name="P10.3/CCU60_COUT60/U0C0_DX2A/U0C1_DX2A/AD3"/>
<pin name="P0.5/U1C1_SCLKOUT/U1C10_SELO2/CCU61_COUT62/U1C1_DX1A/U1C0_DX1C/A5"/>
<pin name="P10.4/U0C0_SELO3/CCU60_COUT61/U0C0_DX2B/U0C1_DX2B/AD4"/>
<pin name="P10.5/U0C1_SCLKOUT/CCU60_COUT62/U0C1_DX1B/AD5"/>
<pin name="P0.6/U1C1_DOUT/TXDC1/CCU61_COUT63/U1C1_DX0A/CCU61_CTRAPA/U1C1_DX1B/A6"/>
<pin name="P10.6/U0C0_DOUT/TXDC4/U1C0_SELO0/U0C0_DX0C/U1C0_DX2D/CCU60_CTRAPA/AD6"/>
<pin name="P10.7/U0C1_DOUT/CCU60_COUT63/U0C1_DX0B/CCU60_CCPOS0A/DXD4C/AD7"/>
<pin name="P0.7/U1C1_DOUT/U1C0_SELO3/U1C1_DX0B/CCU61_CTRAPB/A7"/>
<pin name="VDDPB@6"/>
<pin name="VSS@4"/>
<pin name="VDDPB@7"/>
<pin name="P1.0/U1C0_MCLKOUT/U1C0_SELO4/EX0BINA/CCU62_CTRAPB/A8"/>
<pin name="P10.8/!BRKIN_B/U0C0_DX1C/CCU60_CCPOS1A/U0C1_SELO0/U0C0_MCLKOUT/AD8"/>
<pin name="P10.9/U0C0_SELO4/U0C1_MCLKOUT/CCU60_CCPOS2A/TCK_B/AD9"/>
<pin name="P1.1/CCU62_COUT62/U1C0_SELO5/U2C1_DOUT/EX1BINA/U2C1_DX0C/A9"/>
<pin name="P10.10/TDI_B/U0C1_DX1A/U0C0_DX2C/CCU60_COUT63/U0C0_SELO0/AD10"/>
<pin name="P10.11/U1C0_SCLKOUT/!BRKOUT/U1C0_DX1D/RXDC2B/TMS_B/AD11"/>
<pin name="P1.2/CCU62_CC62/U1C0_SELO6/U2C1_SCLKOUT/CCU61_T12HRB/EX2AINA/A2C1_DX0D/U2C1_DX1C/A10"/>
<pin name="P10.12/U1C0_DOUT/TXDC2/TDO/U1C0_DX0C/U1C0_DX1E/AD12"/>
<pin name="P10.13/U1C0_DOUT/TXDC3/U1C0_SELO3/U1C0_DX0D/!WRL/!WR"/>
<pin name="P1.3/CCU62_COUT63/U1C0_SELO7/U2C0_SELO4/CCU62_T12HRB/EX3AINA/A11"/>
<pin name="VDD@2"/>
<pin name="P10.14/U1C0_SELO1/U0C1_DX0C/RXDC3C/!RD"/>
<pin name="P1.4/CCU62_COUT61/U1C1_SELO4/U2C0_SELO5/U2C0_DX2B/A12"/>
<pin name="P10.15/U1C0_SELO2/U0C1_DOUT/U1C0_DOUT/U0C1_DX1C/ALE"/>
<pin name="P1.5/CCU62_COUT60/U1C1_SELO3/!BRKOUT/U2C0_DX0C/A13"/>
<pin name="P1.6/CCU62_CC61/U1C1_SELO2/U2C0_DOUT/U2C0_DX0D/A14"/>
<pin name="P1.7/CCU62_CC60/U1C1_MCLKOUT/U2C0_SCLKOUT/U2C0_DX1C/A15"/>
<pin name="XTAL2" direction="pwr" function="clk"/>
<pin name="XTAL1" direction="pwr" function="clk"/>
<pin name="/PORST" function="dot"/>
<pin name="ESR1/EX0AINB"/>
<pin name="ESR0"/>
<pin name="VDDPB@1" direction="pwr"/>
</symbol>
<symbol name="TC1100">
<pin name="!NMI" direction="in"/>
<pin name="!RD" direction="out"/>
<pin name="!CS0" direction="out"/>
<pin name="!PORST" direction="in"/>
<pin name="!HDRST"/>
<pin name="HWCFG0" direction="in"/>
<pin name="!WAIT" direction="in"/>
<pin name="ALE" direction="out"/>
<pin name="!BAA" direction="out"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!CS1" direction="out"/>
<pin name="!CS2" direction="out"/>
<pin name="!CS3" direction="out"/>
<pin name="!CSCOMB" direction="out"/>
<pin name="CKE" direction="out"/>
<pin name="SDCLKI" direction="in"/>
<pin name="!ADV" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VDDOSC" direction="in"/>
<pin name="VSSOSC" direction="in"/>
<pin name="RESERVED@1" direction="pas"/>
<pin name="!BC0"/>
<pin name="!BC1"/>
<pin name="!BC2"/>
<pin name="!BC3"/>
<pin name="!RD_WR" direction="out"/>
<pin name="HWCFG1" direction="in"/>
<pin name="HWCFG2" direction="in"/>
<pin name="!TRCLK" direction="out"/>
<pin name="SDCLKO" direction="out"/>
<pin name="BFCLKI" direction="in"/>
<pin name="BFCLKO" direction="out"/>
<pin name="VDDOSC3" direction="in"/>
<pin name="VSSOSC3" direction="in"/>
<pin name="!MR_W" direction="out"/>
<pin name="RESERVED@2" direction="pas"/>
<pin name="RESERVED@3" direction="pas"/>
<pin name="RESERVED@4" direction="pas"/>
<pin name="NC@1" direction="pas"/>
<pin name="NC@2" direction="pas"/>
<pin name="NC@3" direction="pas"/>
<pin name="!BRKIN" direction="in"/>
</symbol>
<symbol name="PORT16">
<pin name="0" direction="in"/>
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="6" direction="in"/>
<pin name="7" direction="in"/>
<pin name="8" direction="in"/>
<pin name="9" direction="in"/>
<pin name="10" direction="in"/>
<pin name="11" direction="in"/>
<pin name="12" direction="in"/>
<pin name="13" direction="in"/>
<pin name="14" direction="in"/>
<pin name="15" direction="in"/>
</symbol>
<symbol name="PORT8">
<pin name="0" direction="in"/>
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="6" direction="in"/>
<pin name="7" direction="in"/>
</symbol>
<symbol name="AD31">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
</symbol>
<symbol name="A23">
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
</symbol>
<symbol name="JTAG">
<pin name="!TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
</symbol>
<symbol name="VSS">
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="VDD">
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="VDDP">
<pin name="VDDP" direction="pwr"/>
</symbol>
<symbol name="TC1130">
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16"/>
<pin name="A17"/>
<pin name="A18"/>
<pin name="A19"/>
<pin name="A20"/>
<pin name="A21"/>
<pin name="A22"/>
<pin name="A23"/>
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="NMI"/>
<pin name="/RD" function="dot"/>
<pin name="/WR" function="dot"/>
<pin name="CS0" function="dot"/>
<pin name="CS1" function="dot"/>
<pin name="CS2" function="dot"/>
<pin name="CS3" function="dot"/>
<pin name="BC0" function="dot"/>
<pin name="BC1" function="dot"/>
<pin name="BC2" function="dot"/>
<pin name="BC3" function="dot"/>
<pin name="/PORST" function="dot"/>
<pin name="/HDRST" function="dot"/>
<pin name="HWCFG0"/>
<pin name="HWCFG1"/>
<pin name="HWCFG2"/>
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="VDDOSC"/>
<pin name="VDDOSC3"/>
<pin name="VSSOSC3"/>
<pin name="VSSOSC"/>
<pin name="/WAIT" function="dot"/>
<pin name="/MR_W" function="dot"/>
<pin name="BFCLKI"/>
<pin name="BFCLKO"/>
<pin name="ALE"/>
<pin name="/BAA" function="dot"/>
<pin name="/ADV" function="dot"/>
<pin name="/CSCOMB" function="dot"/>
<pin name="CKE"/>
<pin name="/RAS" function="dot"/>
<pin name="/CAS" function="dot"/>
<pin name="SDCLKI"/>
<pin name="SDCLKO"/>
<pin name="D+"/>
<pin name="D-"/>
<pin name="TRST"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="/BRKIN" function="dot"/>
<pin name="TRCLK"/>
<pin name="MI_TXCLK"/>
<pin name="MI_RXCLK"/>
<pin name="MI_MDIO"/>
</symbol>
<symbol name="PWR_TC1130">
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDDP@0" direction="pwr"/>
<pin name="VDDP@1" direction="pwr"/>
<pin name="VDDP@2" direction="pwr"/>
<pin name="VDDP@3" direction="pwr"/>
<pin name="VDDP@4" direction="pwr"/>
<pin name="VDDP@5" direction="pwr"/>
</symbol>
<symbol name="NC4">
<pin name="RESERVED@0" direction="nc"/>
<pin name="RESERVED@1" direction="nc"/>
<pin name="RESERVED@2" direction="nc"/>
<pin name="RESERVED@3" direction="nc"/>
</symbol>
<symbol name="TC1762">
<pin name="P5.0" direction="pas"/>
<pin name="P5.1" direction="pas"/>
<pin name="P5.2" direction="pas"/>
<pin name="P5.3" direction="pas"/>
<pin name="P5.4" direction="pas"/>
<pin name="P5.5" direction="pas"/>
<pin name="P5.6" direction="pas"/>
<pin name="P5.7" direction="pas"/>
<pin name="TRCLK" direction="pas"/>
<pin name="P5.8" direction="pas"/>
<pin name="P5.9" direction="pas"/>
<pin name="P5.10" direction="pas"/>
<pin name="P5.11" direction="pas"/>
<pin name="P5.12" direction="pas"/>
<pin name="P5.13" direction="pas"/>
<pin name="P5.14" direction="pas"/>
<pin name="P5.15" direction="pas"/>
<pin name="NC@0" direction="pas"/>
<pin name="AN35" direction="pas"/>
<pin name="AN34" direction="pas"/>
<pin name="AN33" direction="pas"/>
<pin name="AN32" direction="pas"/>
<pin name="AN31" direction="pas"/>
<pin name="AN30" direction="pas"/>
<pin name="AN29" direction="pas"/>
<pin name="AN28" direction="pas"/>
<pin name="AN7" direction="pas"/>
<pin name="AN27" direction="pas"/>
<pin name="AN26" direction="pas"/>
<pin name="AN25" direction="pas"/>
<pin name="AN24" direction="pas"/>
<pin name="AN23" direction="pas"/>
<pin name="AN22" direction="pas"/>
<pin name="AN21" direction="pas"/>
<pin name="AN20" direction="pas"/>
<pin name="AN19" direction="pas"/>
<pin name="AN18" direction="pas"/>
<pin name="AN17" direction="pas"/>
<pin name="AN16" direction="pas"/>
<pin name="AN15" direction="pas"/>
<pin name="AN14" direction="pas"/>
<pin name="AN13" direction="pas"/>
<pin name="AN12" direction="pas"/>
<pin name="AN11" direction="pas"/>
<pin name="AN10" direction="pas"/>
<pin name="AN9" direction="pas"/>
<pin name="AN8" direction="pas"/>
<pin name="AN6" direction="pas"/>
<pin name="AN5" direction="pas"/>
<pin name="AN4" direction="pas"/>
<pin name="AN3" direction="pas"/>
<pin name="AN2" direction="pas"/>
<pin name="AN1" direction="pas"/>
<pin name="AN0" direction="pas"/>
<pin name="P1.14" direction="pas"/>
<pin name="P1.13" direction="pas"/>
<pin name="P1.12" direction="pas"/>
<pin name="P2.0" direction="pas"/>
<pin name="P2.1" direction="pas"/>
<pin name="P2.2" direction="pas"/>
<pin name="P2.3" direction="pas"/>
<pin name="P2.4" direction="pas"/>
<pin name="P2.5" direction="pas"/>
<pin name="P2.6" direction="pas"/>
<pin name="P2.7" direction="pas"/>
<pin name="P4.0" direction="pas"/>
<pin name="P4.1" direction="pas"/>
<pin name="P4.2" direction="pas"/>
<pin name="NC@1" direction="pas"/>
<pin name="P4.3" direction="pas"/>
<pin name="P1.0" direction="pas"/>
<pin name="P1.1" direction="pas"/>
<pin name="P1.2" direction="pas"/>
<pin name="P1.8" direction="pas"/>
<pin name="P1.9" direction="pas"/>
<pin name="P1.10" direction="pas"/>
<pin name="P1.11" direction="pas"/>
<pin name="P1.3" direction="pas"/>
<pin name="XTAL1" direction="pas" function="clk"/>
<pin name="XTAL2" direction="pas" function="clk"/>
<pin name="P1.4" direction="pas"/>
<pin name="P1.5" direction="pas"/>
<pin name="P1.6" direction="pas"/>
<pin name="P1.7" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="/TRST" direction="pas" function="dot"/>
<pin name="TCK" direction="pas"/>
<pin name="/BRKOUT" direction="pas" function="dot"/>
<pin name="/BRKIN" direction="pas" function="dot"/>
<pin name="/TEST_MODE" direction="pas" function="dot"/>
<pin name="BYPASS" direction="pas"/>
<pin name="/NMI" direction="pas" function="dot"/>
<pin name="/PORST" direction="pas" function="dot"/>
<pin name="/HDRST" direction="pas" function="dot"/>
<pin name="P3.5" direction="pas"/>
<pin name="P3.6" direction="pas"/>
<pin name="P3.8" direction="pas"/>
<pin name="P3.2" direction="pas"/>
<pin name="P3.3" direction="pas"/>
<pin name="P3.7" direction="pas"/>
<pin name="P3.4" direction="pas"/>
<pin name="P3.15" direction="pas"/>
<pin name="P3.14" direction="pas"/>
<pin name="P3.1" direction="pas"/>
<pin name="P3.0" direction="pas"/>
<pin name="P3.10" direction="pas"/>
<pin name="P3.9" direction="pas"/>
<pin name="P3.13" direction="pas"/>
<pin name="P3.12" direction="pas"/>
<pin name="P3.11" direction="pas"/>
<pin name="P0.0" direction="pas"/>
<pin name="P0.1" direction="pas"/>
<pin name="P0.2" direction="pas"/>
<pin name="P0.3" direction="pas"/>
<pin name="P0.8" direction="pas"/>
<pin name="P0.9" direction="pas"/>
<pin name="P0.10" direction="pas"/>
<pin name="P0.11" direction="pas"/>
<pin name="FCLN0" direction="pas"/>
<pin name="FCLP0A" direction="pas"/>
<pin name="SON0" direction="pas"/>
<pin name="SOP0A" direction="pas"/>
<pin name="P2.9" direction="pas"/>
<pin name="P2.10" direction="pas"/>
<pin name="P2.11" direction="pas"/>
<pin name="P2.12" direction="pas"/>
<pin name="P2.8" direction="pas"/>
<pin name="P2.13" direction="pas"/>
<pin name="P0.4" direction="pas"/>
<pin name="P0.5" direction="pas"/>
<pin name="P0.12" direction="pas"/>
<pin name="P0.13" direction="pas"/>
<pin name="P0.6" direction="pas"/>
<pin name="P0.7" direction="pas"/>
<pin name="P0.14" direction="pas"/>
<pin name="P0.15" direction="pas"/>
</symbol>
<symbol name="PWR_TC1762">
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VDDP@0" direction="pwr"/>
<pin name="VDDP@1" direction="pwr"/>
<pin name="VDDP@2" direction="pwr"/>
<pin name="VDDP@3" direction="pwr"/>
<pin name="VDDP@4" direction="pwr"/>
<pin name="VDDP@5" direction="pwr"/>
<pin name="VDDP@6" direction="pwr"/>
<pin name="VDDP@7" direction="pwr"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDDM" direction="pwr"/>
<pin name="VSSM" direction="pwr"/>
<pin name="VDDMF" direction="pwr"/>
<pin name="VSSMF" direction="pwr"/>
<pin name="VDDAF" direction="pwr"/>
<pin name="VSSAF" direction="pwr"/>
<pin name="VAREF0" direction="pwr"/>
<pin name="VAGND0" direction="pwr"/>
<pin name="VAREF" direction="pwr"/>
<pin name="VAGND" direction="pwr"/>
<pin name="VDDOSC" direction="pwr"/>
<pin name="VDDOSC3" direction="pwr"/>
<pin name="VSSOSC" direction="pwr"/>
<pin name="VDDFL3" direction="pwr"/>
</symbol>
<symbol name="TC1796JTAG">
<pin name="!TRST" direction="in" function="dot"/>
<pin name="TCK" direction="in" function="clk"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="!BRKIN" direction="in" function="dot"/>
<pin name="!BRKOUT" direction="out" function="dot"/>
<pin name="TDO" direction="out"/>
<pin name="TRCLK" direction="out" function="clk"/>
<pin name="TR.0" direction="out"/>
<pin name="TR.1" direction="out"/>
<pin name="TR.2" direction="out"/>
<pin name="TR.3" direction="out"/>
<pin name="TR.4" direction="out"/>
<pin name="TR.5" direction="out"/>
<pin name="TR.6" direction="out"/>
<pin name="TR.7" direction="out"/>
<pin name="TR.8" direction="out"/>
<pin name="TR.9" direction="out"/>
<pin name="TR.10" direction="out"/>
<pin name="TR.11" direction="out"/>
<pin name="TR.12" direction="out"/>
<pin name="TR.13" direction="out"/>
<pin name="TR.14" direction="out"/>
<pin name="TR.15" direction="out"/>
</symbol>
<symbol name="TC1796-P2">
<pin name="P2.15"/>
<pin name="P2.14"/>
<pin name="P2.2"/>
<pin name="P2.3"/>
<pin name="P2.4"/>
<pin name="P2.5"/>
<pin name="P2.6"/>
<pin name="P2.7"/>
<pin name="P2.8"/>
<pin name="P2.9"/>
<pin name="P2.10"/>
<pin name="P2.11"/>
<pin name="P2.12"/>
<pin name="P2.13"/>
</symbol>
<symbol name="TC1796P3">
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4"/>
<pin name="P3.5"/>
<pin name="P3.6"/>
<pin name="P3.7"/>
<pin name="P3.8"/>
<pin name="P3.9"/>
<pin name="P3.10"/>
<pin name="P3.11"/>
<pin name="P3.12"/>
<pin name="P3.13"/>
<pin name="P3.14"/>
<pin name="P3.15"/>
</symbol>
<symbol name="TC1796P4">
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="P4.8"/>
<pin name="P4.9"/>
<pin name="P4.10"/>
<pin name="P4.11"/>
<pin name="P4.12"/>
<pin name="P4.13"/>
<pin name="P4.14"/>
<pin name="P4.15"/>
</symbol>
<symbol name="TC1796P5">
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.4"/>
<pin name="P5.5"/>
<pin name="P5.6"/>
<pin name="P5.7"/>
</symbol>
<symbol name="TC1796P6">
<pin name="P6.15"/>
<pin name="P6.14"/>
<pin name="P6.13"/>
<pin name="P6.12"/>
<pin name="P6.4"/>
<pin name="P6.5"/>
<pin name="P6.6"/>
<pin name="P6.7"/>
<pin name="P6.8"/>
<pin name="P6.9"/>
<pin name="P6.10"/>
<pin name="P6.11"/>
</symbol>
<symbol name="TC1796PWRD">
<pin name="VDDEBU@0" direction="pwr"/>
<pin name="VDDEBU@1" direction="pwr"/>
<pin name="VDDEBU@2" direction="pwr"/>
<pin name="VDDEBU@3" direction="pwr"/>
<pin name="VDDEBU@4" direction="pwr"/>
<pin name="VDDEBU@5" direction="pwr"/>
<pin name="VDDEBU@6" direction="pwr"/>
<pin name="VDDEBU@7" direction="pwr"/>
<pin name="VDDEBU@8" direction="pwr"/>
<pin name="VDDP@0" direction="pwr"/>
<pin name="VDDP@1" direction="pwr"/>
<pin name="VDDP@2" direction="pwr"/>
<pin name="VDDP@3" direction="pwr"/>
<pin name="VDDP@4" direction="pwr"/>
<pin name="VDDP@5" direction="pwr"/>
<pin name="VDDP@6" direction="pwr"/>
<pin name="VDDP@7" direction="pwr"/>
<pin name="VDDP@8" direction="pwr"/>
<pin name="VDDP@9" direction="pwr"/>
<pin name="VDDP@10" direction="pwr"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDDFL3@0" direction="pwr"/>
<pin name="VDDFL3@1" direction="pwr"/>
<pin name="VDDSBRAM" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
<pin name="VSS@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="VSS@45" direction="pwr"/>
<pin name="VSS@46" direction="pwr"/>
<pin name="VSS@47" direction="pwr"/>
<pin name="VSS@48" direction="pwr"/>
<pin name="VSS@49" direction="pwr"/>
<pin name="VSS@50" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VSS@52" direction="pwr"/>
<pin name="VSS@53" direction="pwr"/>
<pin name="VSS@54" direction="pwr"/>
<pin name="VSS@55" direction="pwr"/>
<pin name="VSS@56" direction="pwr"/>
<pin name="VSS@57" direction="pwr"/>
<pin name="VSS@58" direction="pwr"/>
<pin name="VSS@59" direction="pwr"/>
<pin name="VSS@60" direction="pwr"/>
<pin name="VSS@61" direction="pwr"/>
</symbol>
<symbol name="TC1796PWRA">
<pin name="VFAREF@0" direction="pwr"/>
<pin name="VFAGND@0" direction="pwr"/>
<pin name="VDDMF@0" direction="pwr"/>
<pin name="VSSMF@0" direction="pwr"/>
<pin name="VDDAF@0" direction="pwr"/>
<pin name="VSSAF@0" direction="pwr"/>
<pin name="VAREF@0" direction="pwr"/>
<pin name="VAREF@1" direction="pwr"/>
<pin name="VAGND@0" direction="pwr"/>
<pin name="VAGND@1" direction="pwr"/>
<pin name="VDDM@0" direction="pwr"/>
<pin name="VSSM@0" direction="pwr"/>
</symbol>
<symbol name="TC1796AN">
<pin name="AN0" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AN3" direction="in"/>
<pin name="AN4" direction="in"/>
<pin name="AN5" direction="in"/>
<pin name="AN6" direction="in"/>
<pin name="AN7" direction="in"/>
<pin name="AN8" direction="in"/>
<pin name="AN9" direction="in"/>
<pin name="AN10" direction="in"/>
<pin name="AN11" direction="in"/>
<pin name="AN12" direction="in"/>
<pin name="AN13" direction="in"/>
<pin name="AN14" direction="in"/>
<pin name="AN15" direction="in"/>
<pin name="AN16" direction="in"/>
<pin name="AN17" direction="in"/>
<pin name="AN18" direction="in"/>
<pin name="AN19" direction="in"/>
<pin name="AN20" direction="in"/>
<pin name="AN21" direction="in"/>
<pin name="AN22" direction="in"/>
<pin name="AN23" direction="in"/>
<pin name="AN24" direction="in"/>
<pin name="AN25" direction="in"/>
<pin name="AN26" direction="in"/>
<pin name="AN27" direction="in"/>
<pin name="AN28" direction="in"/>
<pin name="AN29" direction="in"/>
<pin name="AN30" direction="in"/>
<pin name="AN31" direction="in"/>
<pin name="AN32" direction="in"/>
<pin name="AN33" direction="in"/>
<pin name="AN34" direction="in"/>
<pin name="AN35" direction="in"/>
<pin name="AN36" direction="in"/>
<pin name="AN37" direction="in"/>
<pin name="AN38" direction="in"/>
<pin name="AN39" direction="in"/>
<pin name="AN40" direction="in"/>
<pin name="AN41" direction="in"/>
<pin name="AN42" direction="in"/>
<pin name="AN43" direction="in"/>
</symbol>
<symbol name="TC1796">
<pin name="TSTRES" direction="in"/>
<pin name="TESTMODE" direction="in" function="dot"/>
<pin name="!PORST" direction="in" function="dot"/>
<pin name="!HDRST" function="dot"/>
<pin name="!NMI" direction="in" function="dot"/>
<pin name="BYPASS" direction="in"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="in" function="clk"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
<pin name="D16" direction="hiz"/>
<pin name="D17" direction="hiz"/>
<pin name="D18" direction="hiz"/>
<pin name="D19" direction="hiz"/>
<pin name="D20" direction="hiz"/>
<pin name="D21" direction="hiz"/>
<pin name="D22" direction="hiz"/>
<pin name="D23" direction="hiz"/>
<pin name="D24" direction="hiz"/>
<pin name="D25" direction="hiz"/>
<pin name="D26" direction="hiz"/>
<pin name="D27" direction="hiz"/>
<pin name="D28" direction="hiz"/>
<pin name="D29" direction="hiz"/>
<pin name="D30" direction="hiz"/>
<pin name="D31" direction="hiz"/>
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
<pin name="!CSEL0" direction="out" function="dot"/>
<pin name="!CSEL1" direction="out" function="dot"/>
<pin name="!CSEL2" direction="out" function="dot"/>
<pin name="!CSEL3" direction="out" function="dot"/>
<pin name="!CSEL4" direction="out" function="dot"/>
<pin name="!RD" direction="out" function="dot"/>
<pin name="!RD/!WR" direction="out" function="dot"/>
<pin name="!ADV" direction="out" function="dot"/>
<pin name="!MR/!W" direction="out" function="dot"/>
<pin name="!BC3" direction="out" function="dot"/>
<pin name="!BC2" direction="out" function="dot"/>
<pin name="!BC1" direction="out" function="dot"/>
<pin name="!BC0" direction="out" function="dot"/>
<pin name="!WAIT" direction="out" function="dot"/>
<pin name="!BAA" direction="out" function="dot"/>
<pin name="!HOLD" direction="out" function="dot"/>
<pin name="!HLDA" direction="out" function="dot"/>
<pin name="!BREQ" direction="out" function="dot"/>
<pin name="BFLCKO" direction="out"/>
<pin name="BFCLKI" direction="in"/>
<pin name="P0.0"/>
<pin name="P0.1"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P0.8"/>
<pin name="P0.9"/>
<pin name="P0.10"/>
<pin name="P0.11"/>
<pin name="P0.12"/>
<pin name="P0.13"/>
<pin name="P0.14"/>
<pin name="P0.15"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P1.8"/>
<pin name="P1.9"/>
<pin name="P1.10"/>
<pin name="P1.11"/>
<pin name="P1.12"/>
<pin name="P1.13"/>
<pin name="P1.14"/>
<pin name="P1.15"/>
<pin name="P10.0/HWCFG.0"/>
<pin name="P10.1/HWCFG.1"/>
<pin name="P10.2/HWCFG.2"/>
<pin name="P10.3/HWCFG.3"/>
<pin name="P9.0"/>
<pin name="P9.1"/>
<pin name="P9.2"/>
<pin name="P9.3"/>
<pin name="P9.4"/>
<pin name="P9.5"/>
<pin name="P9.6"/>
<pin name="P9.7"/>
<pin name="P9.8"/>
<pin name="P8.0"/>
<pin name="P8.1"/>
<pin name="P8.2"/>
<pin name="P8.3"/>
<pin name="P8.4"/>
<pin name="P8.5"/>
<pin name="P8.6"/>
<pin name="P8.7"/>
<pin name="P7.0"/>
<pin name="P7.1"/>
<pin name="P7.2"/>
<pin name="P7.3"/>
<pin name="P7.4"/>
<pin name="P7.5"/>
<pin name="P7.6"/>
<pin name="P7.7"/>
<pin name="SON1" direction="out"/>
<pin name="SOP1A" direction="out"/>
<pin name="FCLN1" direction="out"/>
<pin name="FCLP1A" direction="out"/>
<pin name="SON0" direction="out"/>
<pin name="SOP0A" direction="out"/>
<pin name="FCLN0" direction="out"/>
<pin name="FCLP0A" direction="out"/>
<pin name="SLSIO"/>
<pin name="SCLK0"/>
<pin name="MRST0"/>
<pin name="MTSR0"/>
<pin name="SLSO1"/>
<pin name="SLSO0"/>
<pin name="VDDOSC-3V" direction="nc"/>
<pin name="VDDOSC-1.5V" direction="nc"/>
<pin name="VSSOSC" direction="nc"/>
</symbol>
<symbol name="TC1796NC">
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
</symbol>
<symbol name="TC1910">
<pin name="!RD" function="dot"/>
<pin name="!CS0" direction="out" function="dot"/>
<pin name="!PORST" direction="in" function="dot"/>
<pin name="CLKOUT" direction="out"/>
<pin name="!WAIT" function="dot"/>
<pin name="!MR_W" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!BAA" direction="out" function="dot"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!CS1" direction="out" function="dot"/>
<pin name="!CS2" direction="out" function="dot"/>
<pin name="!CS3" direction="out" function="dot"/>
<pin name="!CS4" direction="out" function="dot"/>
<pin name="!CS5" direction="out" function="dot"/>
<pin name="!CS6" direction="out" function="dot"/>
<pin name="!CSGLB" direction="out" function="dot"/>
<pin name="CKE" direction="out"/>
<pin name="EBUCLK" direction="out"/>
<pin name="!ADV" direction="out" function="dot"/>
<pin name="!CMDELAY" direction="in" function="dot"/>
<pin name="!SCANMODE" direction="in" function="dot"/>
<pin name="TM_CTRL0" direction="in"/>
<pin name="TM_CTRL1" direction="in"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="out" function="clk"/>
<pin name="!BC0" function="dot"/>
<pin name="!BC1" function="dot"/>
<pin name="!BC2" function="dot"/>
<pin name="!BC3" function="dot"/>
<pin name="!RD_WR" function="dot"/>
<pin name="BFCLK0" direction="out"/>
<pin name="AI0+" direction="in"/>
<pin name="AI0-" direction="in"/>
<pin name="AO0+" direction="out"/>
<pin name="AO0-" direction="out"/>
<pin name="AI1+" direction="in"/>
<pin name="AI1-" direction="in"/>
<pin name="AO1+" direction="out"/>
<pin name="AO1-" direction="out"/>
<pin name="CEXT" direction="in"/>
<pin name="CODEC_DIS" direction="in"/>
<pin name="!CSEMU" direction="out" function="dot"/>
<pin name="!CSOVL" direction="out" function="dot"/>
<pin name="PLLCTRL_AO" direction="in"/>
<pin name="XTAL3" direction="in" function="clk"/>
<pin name="XTAL4" direction="out" function="clk"/>
<pin name="VAREF_GOD" direction="in"/>
<pin name="VAGND_GOD" direction="in"/>
<pin name="VDD_COD0/1" direction="in"/>
<pin name="VSSA_COD0/1" direction="in"/>
<pin name="VDD_GUARD" direction="in"/>
<pin name="VSS_GUARD" direction="in"/>
<pin name="VDD_OSCI" direction="in"/>
<pin name="VDD_RTC" direction="in"/>
<pin name="VSS_32K" direction="in"/>
<pin name="VDD_PLL" direction="in"/>
<pin name="VSS_PLL" direction="in"/>
<pin name="VDDPLL" direction="in"/>
<pin name="VSSPLL" direction="in"/>
<pin name="VDDR" direction="in"/>
<pin name="VDDSB" direction="in"/>
<pin name="VDD_PWR@1" direction="in"/>
<pin name="VDD_PWR@2" direction="in"/>
<pin name="VDD_PWR@3" direction="in"/>
<pin name="VDD_PWR@4" direction="in"/>
<pin name="VDD_PWR@5" direction="in"/>
<pin name="VDD_PWR2@1" direction="in"/>
<pin name="VDD_PWR2@2" direction="in"/>
<pin name="VDD_PWR2@3" direction="in"/>
<pin name="VDD_PWR2@4" direction="in"/>
<pin name="VSS_GND@1" direction="in"/>
<pin name="VSS_GND@2" direction="in"/>
<pin name="VSS_GND@3" direction="in"/>
<pin name="VSS_GND@4" direction="in"/>
<pin name="VSS_GND@5" direction="in"/>
<pin name="VSS_GND@6" direction="in"/>
<pin name="!NMI" direction="in" function="dot"/>
<pin name="BYPASS" direction="in"/>
<pin name="!HRST" function="dot"/>
</symbol>
<symbol name="JTAG-OCSD">
<pin name="!TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="!OCDSE" direction="in"/>
<pin name="!BRKIN" direction="in"/>
<pin name="!BRKOUT" direction="out"/>
</symbol>
<symbol name="PORT0-10_12">
<pin name="0/EXI0IN"/>
<pin name="1/EXI1IN/DATA_IN"/>
<pin name="2/EXI2IN/DATA_OUT"/>
<pin name="3/EXI3IN/MCLK"/>
<pin name="4/GPIO/SCLK"/>
<pin name="5/GPIO/LRCK"/>
<pin name="6/GPIO/MUTE0"/>
<pin name="7/GPIO/MUTE1"/>
</symbol>
<symbol name="PORT1-10_12">
<pin name="0/GPIO"/>
<pin name="1/GPIO"/>
<pin name="2/GPIO"/>
<pin name="3/GPIO"/>
<pin name="4/GPIO"/>
<pin name="5/GPIO"/>
<pin name="6/GPIO"/>
<pin name="7/GPIO"/>
</symbol>
<symbol name="PORT2-10_12">
<pin name="0/GPIO/RXDCAN0"/>
<pin name="1/GPIO/TXDCAN0"/>
<pin name="2/GPIO/RXDCAN1"/>
<pin name="3/GPIO/TXDCAN1"/>
<pin name="4/GPIO"/>
<pin name="5/GPIO"/>
<pin name="6/SCL"/>
<pin name="7/SDA"/>
<pin name="8/GPIO"/>
<pin name="9/GPIO"/>
<pin name="10/RXD0"/>
<pin name="11/TXD0"/>
<pin name="12/SCLK"/>
<pin name="13/MRST"/>
<pin name="14/MTSR"/>
<pin name="15/GPIO/EXI4IN/PLL_CLC.LOCK"/>
</symbol>
<symbol name="PORT3-10_12">
<pin name="0/GPTU.0"/>
<pin name="1/GPTU.1"/>
<pin name="2/GPTU.2"/>
<pin name="3/GPTU.3"/>
<pin name="4/GPTU.4"/>
<pin name="5/GPTU.5"/>
<pin name="6/GPTU.6"/>
<pin name="7/GPTU.7"/>
<pin name="8/RXD1"/>
<pin name="9/TXD1"/>
<pin name="10/GPIO/RXD2"/>
<pin name="11/GPIO/OSCBYP/TXD2"/>
<pin name="12/EXI5IN/HWCFG0"/>
<pin name="13/EXI6IN/HWCFG1"/>
<pin name="14/EXI7IN/HWCFG2"/>
<pin name="15/GPIO"/>
</symbol>
<symbol name="HEATSINK">
<pin name="HS" direction="in"/>
</symbol>
<symbol name="JTAG-OCSD-1">
<pin name="!TRST" direction="in" function="dot"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="!OCDSE" direction="in" function="dot"/>
<pin name="!BRKIN" direction="in" function="dot"/>
<pin name="!BRKOUT" direction="out" function="dot"/>
</symbol>
<symbol name="D31">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="D16"/>
<pin name="D17"/>
<pin name="D18"/>
<pin name="D19"/>
<pin name="D20"/>
<pin name="D21"/>
<pin name="D22"/>
<pin name="D23"/>
<pin name="D24"/>
<pin name="D25"/>
<pin name="D26"/>
<pin name="D27"/>
<pin name="D28"/>
<pin name="D29"/>
<pin name="D30"/>
<pin name="D31"/>
</symbol>
<symbol name="TC1920PWR">
<pin name="1V8@0" direction="pwr"/>
<pin name="1V8@1" direction="pwr"/>
<pin name="1V8@2" direction="pwr"/>
<pin name="1V8@3" direction="pwr"/>
<pin name="1V8@4" direction="pwr"/>
<pin name="1V8@5" direction="pwr"/>
<pin name="1V8@6" direction="pwr"/>
<pin name="1V8@7" direction="pwr"/>
<pin name="3V3@0" direction="pwr"/>
<pin name="3V3@1" direction="pwr"/>
<pin name="3V3@2" direction="pwr"/>
<pin name="3V3@3" direction="pwr"/>
<pin name="3V3@4" direction="pwr"/>
<pin name="3V3@5" direction="pwr"/>
<pin name="3V3@6" direction="pwr"/>
<pin name="3V3@7" direction="pwr"/>
<pin name="3V3@8" direction="pwr"/>
<pin name="3V3@9" direction="pwr"/>
<pin name="3V3@10" direction="pwr"/>
<pin name="3V3@11" direction="pwr"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pwr"/>
<pin name="GND@22" direction="pwr"/>
<pin name="GND@23" direction="pwr"/>
<pin name="GND@24" direction="pwr"/>
<pin name="GND@25" direction="pwr"/>
<pin name="GND@26" direction="pwr"/>
<pin name="GND@27" direction="pwr"/>
<pin name="GND@28" direction="pwr"/>
</symbol>
<symbol name="TC1920PWR2">
<pin name="VDDR@0" direction="pwr"/>
<pin name="VDDR@1" direction="pwr"/>
<pin name="VDD_SB" direction="pwr"/>
<pin name="VDD_GUARD" direction="pwr"/>
<pin name="VSS_GUARD@1" direction="pwr"/>
<pin name="VSS_GUARD@2" direction="pwr"/>
<pin name="VGND_COD" direction="pwr"/>
<pin name="VREF_COD" direction="pwr"/>
<pin name="VSSP_COD@0" direction="pwr"/>
<pin name="VSSP_OSC@0" direction="pwr"/>
<pin name="VSSA_COD@0" direction="pwr"/>
<pin name="VSSP_OSC@1" direction="pwr"/>
<pin name="VDDP_COD@0" direction="pwr"/>
<pin name="VDDP_OSC@1" direction="pwr"/>
<pin name="VAGND_ADC" direction="pwr"/>
<pin name="VAREF_ADC" direction="pwr"/>
<pin name="VSSA_ADC" direction="pwr"/>
<pin name="VSSP_ADC@0" direction="pwr"/>
<pin name="VSSP_ADC@1" direction="pwr"/>
<pin name="VSSP_ADC@2" direction="pwr"/>
<pin name="VDDP_ADC" direction="pwr"/>
<pin name="VSS_PLL" direction="pwr"/>
<pin name="VDD_PLL" direction="pwr"/>
</symbol>
<symbol name="TC1920">
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="XTAL3" function="clk"/>
<pin name="XTAL4" function="clk"/>
<pin name="CLKOUT" direction="out" function="clk"/>
<pin name="HRST" function="dot"/>
<pin name="PORST" direction="in" function="dot"/>
<pin name="NMI" direction="in" function="dot"/>
<pin name="BYPASS" direction="in"/>
<pin name="VDD_OSC2" direction="pwr"/>
<pin name="VDD_OSC1" direction="pwr"/>
<pin name="VDDP_OSC" direction="pwr"/>
<pin name="VSS_OSC" direction="pwr"/>
<pin name="CS0" function="dot"/>
<pin name="CS1" function="dot"/>
<pin name="CS2" function="dot"/>
<pin name="CS3" function="dot"/>
<pin name="CS4" function="dot"/>
<pin name="CS5" function="dot"/>
<pin name="CS6" function="dot"/>
<pin name="CSEMU" function="dot"/>
<pin name="CSOVL" function="dot"/>
<pin name="/BC0" function="dot"/>
<pin name="/BC1" function="dot"/>
<pin name="/BC2" function="dot"/>
<pin name="/BC3" function="dot"/>
<pin name="/RD" function="dot"/>
<pin name="/WR" function="dot"/>
<pin name="ALE"/>
<pin name="/WAIT" function="dot"/>
<pin name="/BAA" function="dot"/>
<pin name="EBUCLK"/>
<pin name="BFCLK0"/>
<pin name="/CSGLB" function="dot"/>
<pin name="/CMDELAY" function="dot"/>
<pin name="MR/W" function="dot"/>
<pin name="CKE"/>
<pin name="/RAS" function="dot"/>
<pin name="/CAS" function="dot"/>
<pin name="P4.0/AIN0"/>
<pin name="P4.1/AIN1"/>
<pin name="P4.2/AIN2"/>
<pin name="P4.3/AIN3"/>
<pin name="P4.4/AIN4"/>
<pin name="P4.5/AIN5"/>
<pin name="/SCAN_MODE" function="dot"/>
<pin name="PLLCTRL_A0"/>
<pin name="TM_CTRL0"/>
<pin name="TM_CTRL1"/>
<pin name="AI0+"/>
<pin name="AI0-"/>
<pin name="AO0+"/>
<pin name="AO0-"/>
<pin name="AI1+"/>
<pin name="AI1-"/>
<pin name="AO1+"/>
<pin name="AO1-"/>
<pin name="CEXT"/>
<pin name="CODEC_DIS"/>
<pin name="/ADV" direction="pwr" function="dot"/>
</symbol>
<symbol name="TC10">
<pin name="A0" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A2" direction="out"/>
<pin name="A3" direction="out"/>
<pin name="A4" direction="out"/>
<pin name="A5" direction="out"/>
<pin name="A6" direction="out"/>
<pin name="A7" direction="out"/>
<pin name="A8" direction="out"/>
<pin name="A9" direction="out"/>
<pin name="A10" direction="out"/>
<pin name="A11" direction="out"/>
<pin name="A12" direction="out"/>
<pin name="A13" direction="out"/>
<pin name="A14" direction="out"/>
<pin name="A15" direction="out"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="A21" direction="out"/>
<pin name="A22" direction="out"/>
<pin name="A23" direction="out"/>
<pin name="AD0"/>
<pin name="AD1"/>
<pin name="AD2"/>
<pin name="AD3"/>
<pin name="AD4"/>
<pin name="AD5"/>
<pin name="AD6"/>
<pin name="AD7"/>
<pin name="AD8"/>
<pin name="AD9"/>
<pin name="AD10"/>
<pin name="AD11"/>
<pin name="AD12"/>
<pin name="AD13"/>
<pin name="AD14"/>
<pin name="AD15"/>
<pin name="AD16"/>
<pin name="AD17"/>
<pin name="AD18"/>
<pin name="AD19"/>
<pin name="AD20"/>
<pin name="AD21"/>
<pin name="AD22"/>
<pin name="AD23"/>
<pin name="AD24"/>
<pin name="AD25"/>
<pin name="AD26"/>
<pin name="AD27"/>
<pin name="AD28"/>
<pin name="AD29"/>
<pin name="AD30"/>
<pin name="AD31"/>
<pin name="XTAL1" direction="in" function="clk"/>
<pin name="XTAL2" direction="out" function="clk"/>
<pin name="P0.1"/>
<pin name="P0.2"/>
<pin name="P0.3"/>
<pin name="P0.4"/>
<pin name="P0.5"/>
<pin name="P0.6"/>
<pin name="P0.7"/>
<pin name="P0.0"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P2.0"/>
<pin name="P2.1"/>
<pin name="P2.2"/>
<pin name="P2.3"/>
<pin name="P2.4"/>
<pin name="P2.5"/>
<pin name="P2.6"/>
<pin name="P2.7"/>
<pin name="/RD" direction="out" function="dot"/>
<pin name="/WR" direction="out" function="dot"/>
<pin name="/BREQ" direction="out" function="dot"/>
<pin name="/HOLD" direction="out" function="dot"/>
<pin name="/HLDA" direction="out" function="dot"/>
<pin name="ALE" direction="out"/>
<pin name="NMI" direction="in" function="dot"/>
<pin name="/HRST" direction="in" function="dot"/>
<pin name="/POR" direction="in" function="dot"/>
<pin name="/CODE" direction="out" function="dot"/>
<pin name="/CAS" direction="out" function="dot"/>
<pin name="/RAS" direction="out" function="dot"/>
<pin name="/CSFPI" direction="out" function="dot"/>
<pin name="/WAIT" direction="out" function="dot"/>
<pin name="/CSOL" direction="out" function="dot"/>
<pin name="/CSFM" direction="out" function="dot"/>
<pin name="EBUC" direction="out"/>
<pin name="STATUS0"/>
<pin name="STATUS1"/>
<pin name="STATUS2"/>
<pin name="STATUS3"/>
<pin name="STATUS4"/>
<pin name="BRKPT0"/>
<pin name="BRKPT1"/>
<pin name="BRKPT2"/>
<pin name="IND_PC0"/>
<pin name="IND_PC1"/>
<pin name="IND_PC2"/>
<pin name="IND_PC3"/>
<pin name="IND_PC4"/>
<pin name="IND_PC5"/>
<pin name="IND_PC6"/>
<pin name="IND_PC7"/>
<pin name="PCP_PC0"/>
<pin name="PCP_PC1"/>
<pin name="PCP_PC2"/>
<pin name="PCP_PC3"/>
<pin name="PCP_PC4"/>
<pin name="PCP_PC5"/>
<pin name="PCP_PC6"/>
<pin name="PCP_PC7"/>
<pin name="PCP_PC8"/>
<pin name="BC0"/>
<pin name="BC1"/>
<pin name="BC2"/>
<pin name="BC3"/>
<pin name="CS0" direction="out" function="dot"/>
<pin name="CS1" direction="out" function="dot"/>
<pin name="CS2" direction="out" function="dot"/>
<pin name="CS3" direction="out" function="dot"/>
<pin name="CLKS@0" direction="in" function="clk"/>
<pin name="CLKS@1" direction="in" function="clk"/>
<pin name="CLKS@2" direction="in" function="clk"/>
<pin name="SCAN@0" direction="in"/>
<pin name="SCAN@1" direction="in"/>
<pin name="VCOS" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TRST" direction="in" function="dot"/>
<pin name="BYPASS"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="OCDS_E" direction="out" function="dot"/>
<pin name="BRK_OUT" direction="out" function="dot"/>
<pin name="(CHIPZ)"/>
</symbol>
<symbol name="VSSE_VDD">
<pin name="VDDE" direction="pwr"/>
<pin name="VSSE" direction="pwr"/>
</symbol>
<symbol name="VSS_VDD">
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="VSSP_VDD">
<pin name="VDDP" direction="pwr"/>
<pin name="VSSP" direction="pwr"/>
</symbol>
<symbol name="TC11IB">
<pin name="CPUCLK" direction="out"/>
<pin name="!NMI" direction="in"/>
<pin name="!RD"/>
<pin name="RESERVED@2"/>
<pin name="!CS0" direction="out"/>
<pin name="!PORST" direction="in"/>
<pin name="!HDRST"/>
<pin name="CFG0"/>
<pin name="!WAIT"/>
<pin name="!MR_W" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!BAA" direction="out"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!CS1" direction="out"/>
<pin name="!CS2" direction="out"/>
<pin name="!CS3" direction="out"/>
<pin name="!CS4" direction="out"/>
<pin name="!CS5" direction="out"/>
<pin name="!CS6" direction="out"/>
<pin name="RESERVED@1" direction="out"/>
<pin name="CFG1"/>
<pin name="CFG2"/>
<pin name="CFG3"/>
<pin name="!SVM" direction="out"/>
<pin name="!HLDA"/>
<pin name="!BREQ" direction="out"/>
<pin name="!CSEMU" direction="out"/>
<pin name="!CSGLB" direction="out"/>
<pin name="!CSOVL" direction="out"/>
<pin name="!CSFPI" direction="out"/>
<pin name="!CKE" direction="out"/>
<pin name="!RMW" direction="out"/>
<pin name="!HOLD" direction="in"/>
<pin name="EBUCLK" direction="out"/>
<pin name="!ADV" direction="out"/>
<pin name="ACLK" direction="out"/>
<pin name="!CMDELAY" direction="in"/>
<pin name="MII_TXCLK" direction="in"/>
<pin name="MII_RXCLK" direction="in"/>
<pin name="MII_MDIO" direction="in"/>
<pin name="TESTMODE" direction="in"/>
<pin name="!TM_CTRL1" direction="in"/>
<pin name="!TM_CTRL2" direction="in"/>
<pin name="CLK42" direction="in"/>
<pin name="PLL96_CTRL" direction="out"/>
<pin name="PLL42_CTRL" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="VDDOSC" direction="in"/>
<pin name="VSSOSC" direction="in"/>
<pin name="VDDPLL96" direction="in"/>
<pin name="VSSPLL96" direction="in"/>
<pin name="VDDPLL42" direction="in"/>
<pin name="VSSPLL42" direction="in"/>
<pin name="VLMUREF" direction="in"/>
<pin name="VCOMREF" direction="in"/>
<pin name="!OCDSE" direction="in"/>
<pin name="!BRKIN" direction="in"/>
<pin name="!BRKOUT" direction="out"/>
<pin name="RESERVED@3"/>
<pin name="VDDDRAM@1" direction="in"/>
<pin name="VDDDRAM@2" direction="in"/>
<pin name="RESERVED@4"/>
<pin name="RESERVED@5"/>
<pin name="!BC0"/>
<pin name="!BC1"/>
<pin name="!BC2"/>
<pin name="!BC3"/>
<pin name="!RDWR"/>
</symbol>
<symbol name="PCI">
<pin name="P_PAR"/>
<pin name="!P_SERR"/>
<pin name="!P_PERR"/>
<pin name="!P_STOP"/>
<pin name="!P_DEVSEL"/>
<pin name="!P_TRDY"/>
<pin name="!P_FRAME"/>
<pin name="!P_IRDY"/>
<pin name="!P_LOCK"/>
<pin name="!P_INTA" direction="out"/>
<pin name="!P_INTB" direction="out"/>
<pin name="!P_PME" direction="out"/>
<pin name="!P_REQ" direction="out"/>
<pin name="!P_GNT" direction="in"/>
<pin name="P_IDSEL" direction="in"/>
<pin name="P_CLK33" direction="in"/>
<pin name="!P_CBE0"/>
<pin name="!P_CBE1"/>
<pin name="!P_CBE2"/>
<pin name="!P_CBE3"/>
</symbol>
<symbol name="ODCS/JTAG">
<pin name="!TRST" direction="in"/>
<pin name="OCDS2PS0" direction="out"/>
<pin name="OCDS2PS1" direction="out"/>
<pin name="OCDS2PS2" direction="out"/>
<pin name="OCDS2PS3" direction="out"/>
<pin name="OCDS2PS4" direction="out"/>
<pin name="OCDS2PC0" direction="out"/>
<pin name="OCDS2PC1" direction="out"/>
<pin name="OCDS2PC2" direction="out"/>
<pin name="OCDS2BRK0" direction="out"/>
<pin name="OCDS2BRK1" direction="out"/>
<pin name="OCDS2BRK2" direction="out"/>
<pin name="OCDS2PC3" direction="out"/>
<pin name="OCDS2PC4" direction="out"/>
<pin name="OCDS2PC5" direction="out"/>
<pin name="OCDS2PC6" direction="out"/>
<pin name="OCDS2PC7" direction="out"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
</symbol>
<symbol name="TC1910-1">
<pin name="!RD"/>
<pin name="!CS0" direction="out"/>
<pin name="!PORST" direction="in"/>
<pin name="CLKOUT" direction="out"/>
<pin name="!WAIT"/>
<pin name="!MR_W" direction="out"/>
<pin name="ALE" direction="out"/>
<pin name="!BAA" direction="out"/>
<pin name="!RAS" direction="out"/>
<pin name="!CAS" direction="out"/>
<pin name="!CS1" direction="out"/>
<pin name="!CS2" direction="out"/>
<pin name="!CS3" direction="out"/>
<pin name="!CS4" direction="out"/>
<pin name="!CS5" direction="out"/>
<pin name="!CS6" direction="out"/>
<pin name="!CSGLB" direction="out"/>
<pin name="CKE" direction="out"/>
<pin name="EBUCLK" direction="out"/>
<pin name="!ADV" direction="out"/>
<pin name="!CMDELAY" direction="in"/>
<pin name="!SCANMODE" direction="in"/>
<pin name="TM_CTRL0" direction="in"/>
<pin name="TM_CTRL1" direction="in"/>
<pin name="XTAL1" direction="in"/>
<pin name="XTAL2" direction="out"/>
<pin name="!BC0"/>
<pin name="!BC1"/>
<pin name="!BC2"/>
<pin name="!BC3"/>
<pin name="!RD_WR"/>
<pin name="BFCLK0" direction="out"/>
<pin name="AI0+" direction="in"/>
<pin name="AI0-" direction="in"/>
<pin name="AO0+" direction="out"/>
<pin name="AO0-" direction="out"/>
<pin name="AI1+" direction="in"/>
<pin name="AI1-" direction="in"/>
<pin name="AO1+" direction="out"/>
<pin name="AO1-" direction="out"/>
<pin name="CEXT" direction="in"/>
<pin name="CODEC_DIS" direction="in"/>
<pin name="!CSEMU" direction="out"/>
<pin name="!CSOVL" direction="out"/>
<pin name="PLLCTRL_AO" direction="in"/>
<pin name="XTAL3" direction="in"/>
<pin name="XTAL4" direction="out"/>
<pin name="VAREF_GOD" direction="in"/>
<pin name="VAGND_GOD" direction="in"/>
<pin name="VDD_COD0/1" direction="in"/>
<pin name="VSSA_COD0/1" direction="in"/>
<pin name="VDD_GUARD" direction="in"/>
<pin name="VSS_GUARD" direction="in"/>
<pin name="VDD_OSCI" direction="in"/>
<pin name="VDD_RTC" direction="in"/>
<pin name="VSS_32K" direction="in"/>
<pin name="VDD_PLL" direction="in"/>
<pin name="VSS_PLL" direction="in"/>
<pin name="VDDPLL" direction="in"/>
<pin name="VSSPLL" direction="in"/>
<pin name="VDDR" direction="in"/>
<pin name="VDDSB" direction="in"/>
<pin name="VDD_PWR@1" direction="in"/>
<pin name="VDD_PWR@2" direction="in"/>
<pin name="VDD_PWR@3" direction="in"/>
<pin name="VDD_PWR@4" direction="in"/>
<pin name="VDD_PWR@5" direction="in"/>
<pin name="VDD_PWR2@1" direction="in"/>
<pin name="VDD_PWR2@2" direction="in"/>
<pin name="VDD_PWR2@3" direction="in"/>
<pin name="VDD_PWR2@4" direction="in"/>
<pin name="VSS_GND@1" direction="in"/>
<pin name="VSS_GND@2" direction="in"/>
<pin name="VSS_GND@3" direction="in"/>
<pin name="VSS_GND@4" direction="in"/>
<pin name="VSS_GND@5" direction="in"/>
<pin name="VSS_GND@6" direction="in"/>
<pin name="!NMI" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="!HRST"/>
</symbol>
<symbol name="AN23">
<pin name="AN0" direction="in"/>
<pin name="AN1" direction="in"/>
<pin name="AN2" direction="in"/>
<pin name="AN3" direction="in"/>
<pin name="AN4" direction="in"/>
<pin name="AN5" direction="in"/>
<pin name="AN6" direction="in"/>
<pin name="AN7" direction="in"/>
<pin name="AN8" direction="in"/>
<pin name="AN9" direction="in"/>
<pin name="AN10" direction="in"/>
<pin name="AN11" direction="in"/>
<pin name="AN12" direction="in"/>
<pin name="AN13" direction="in"/>
<pin name="AN14" direction="in"/>
<pin name="AN15" direction="in"/>
<pin name="AN16" direction="in"/>
<pin name="AN17" direction="in"/>
<pin name="AN18" direction="in"/>
<pin name="AN19" direction="in"/>
<pin name="AN20" direction="in"/>
<pin name="AN21" direction="in"/>
<pin name="AN22" direction="in"/>
<pin name="AN23" direction="in"/>
</symbol>
<symbol name="TC1765">
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="ECIN"/>
<pin name="ECOUT"/>
<pin name="RD" function="dot"/>
<pin name="RD/!WR" function="dot"/>
<pin name="ADV" function="dot"/>
<pin name="/BC0" function="dot"/>
<pin name="/BC1" function="dot"/>
<pin name="/BC2" function="dot"/>
<pin name="/BC3" function="dot"/>
<pin name="/BAA" function="dot"/>
<pin name="/CODE" function="dot"/>
<pin name="/CS0" function="dot"/>
<pin name="/CS1" function="dot"/>
<pin name="/CS2" function="dot"/>
<pin name="/CS3" function="dot"/>
<pin name="/WAIT/!IND" function="dot"/>
<pin name="/CDEMU/!CSOVK" function="dot"/>
<pin name="CPUCLK" function="clk"/>
<pin name="/NMI" function="dot"/>
<pin name="/TEST/MODE" function="dot"/>
<pin name="/HDRST" function="dot"/>
<pin name="BYPASS"/>
<pin name="/PO_RST" function="dot"/>
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.4"/>
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
</symbol>
<symbol name="GND6">
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
</symbol>
<symbol name="NC10">
<pin name="NC@0" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="NC@9" direction="nc"/>
</symbol>
<symbol name="TC1775">
<pin name="XTAL1" function="clk"/>
<pin name="XTAL2" function="clk"/>
<pin name="XTAL3" function="clk"/>
<pin name="XTAL4" function="clk"/>
<pin name="TESTMODE" function="dot"/>
<pin name="CLKIN" direction="in" function="clk"/>
<pin name="CLKOUT" direction="out" function="clk"/>
<pin name="HDRST" function="dot"/>
<pin name="PORST" direction="in" function="dot"/>
<pin name="NMI" direction="in" function="dot"/>
<pin name="CFG0" direction="in"/>
<pin name="CFG1" direction="in"/>
<pin name="CFG2" direction="in"/>
<pin name="CFG3" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="CLKSEL0" direction="in"/>
<pin name="CLKSEL1" direction="in"/>
<pin name="CLKSEL2" direction="in"/>
<pin name="VDD@0" direction="pwr"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VAREF@0" direction="pwr"/>
<pin name="VAREF@1" direction="pwr"/>
<pin name="VAGND@0" direction="pwr"/>
<pin name="VAGND@1" direction="pwr"/>
<pin name="VDDA@0" direction="pwr"/>
<pin name="VDDA@1" direction="pwr"/>
<pin name="VSSA@0" direction="pwr"/>
<pin name="VSSA@1" direction="pwr"/>
</symbol>
<symbol name="TDA6060">
<pin name="AUDGND" direction="pwr"/>
<pin name="AUDINFM" direction="in"/>
<pin name="AUDINAM" direction="in"/>
<pin name="SC2IN" direction="in"/>
<pin name="CAS" direction="in"/>
<pin name="MODOUT1" direction="out"/>
<pin name="MODGND" direction="pwr"/>
<pin name="MODOUT2" direction="out"/>
<pin name="GNDD" direction="pwr"/>
<pin name="SDA" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="VCCD" direction="pwr"/>
<pin name="Q" direction="pas"/>
<pin name="QX" direction="pas"/>
<pin name="P2/ADC" direction="in"/>
<pin name="CHGPMP" direction="in"/>
<pin name="VTUNE" direction="in"/>
<pin name="T1" direction="in"/>
<pin name="O-B1" direction="in"/>
<pin name="O-C2" direction="pas"/>
<pin name="O-C1" direction="pas"/>
<pin name="O-B2" direction="in"/>
<pin name="GNDA" direction="pwr"/>
<pin name="VIDIN" direction="in"/>
<pin name="SLF" direction="pas"/>
<pin name="TFLF" direction="pas"/>
<pin name="T2" direction="pas"/>
<pin name="VCCA" direction="pwr"/>
</symbol>
<symbol name="TLE6361G">
<pin name="/CS" function="dot"/>
<pin name="/ERR" function="dot"/>
<pin name="BOOST"/>
<pin name="BOOTSTRAP"/>
<pin name="C+"/>
<pin name="C-"/>
<pin name="CCP"/>
<pin name="CLK" function="clk"/>
<pin name="DI"/>
<pin name="DO"/>
<pin name="FB/L_IN@0"/>
<pin name="FB/L_IN@1"/>
<pin name="GND@0" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="IN@0"/>
<pin name="IN@1"/>
<pin name="Q_LDO1"/>
<pin name="Q_LDO2"/>
<pin name="Q_LDO3"/>
<pin name="Q_STB"/>
<pin name="Q_T1"/>
<pin name="Q_T2"/>
<pin name="Q_T3"/>
<pin name="Q_T4"/>
<pin name="Q_T5"/>
<pin name="Q_T6"/>
<pin name="R1"/>
<pin name="R2"/>
<pin name="R3"/>
<pin name="SEL"/>
<pin name="SLEW"/>
<pin name="SWQ0"/>
<pin name="SWQ1"/>
<pin name="WAKE"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="80C166" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C166"/>
<gate name="P" symbol="6_VCCVSS"/>
</gates>
<devices>
<device name="" package="MQFP100">
<connects>
<connect gate="G$1" pin="!BUSACT" pad="22"/>
<connect gate="G$1" pin="!NMI" pad="29"/>
<connect gate="G$1" pin="!RD" pad="26"/>
<connect gate="G$1" pin="!RSTIN" pad="27"/>
<connect gate="G$1" pin="!RSTOUT" pad="28"/>
<connect gate="G$1" pin="ALE" pad="25"/>
<connect gate="G$1" pin="EBC0" pad="24"/>
<connect gate="G$1" pin="EBC1" pad="23"/>
<connect gate="G$1" pin="P0-0" pad="98"/>
<connect gate="G$1" pin="P0-1" pad="99"/>
<connect gate="G$1" pin="P0-10" pad="10"/>
<connect gate="G$1" pin="P0-11" pad="11"/>
<connect gate="G$1" pin="P0-12" pad="12"/>
<connect gate="G$1" pin="P0-13" pad="13"/>
<connect gate="G$1" pin="P0-14" pad="14"/>
<connect gate="G$1" pin="P0-15" pad="15"/>
<connect gate="G$1" pin="P0-2" pad="100"/>
<connect gate="G$1" pin="P0-3" pad="1"/>
<connect gate="G$1" pin="P0-4" pad="2"/>
<connect gate="G$1" pin="P0-5" pad="3"/>
<connect gate="G$1" pin="P0-6" pad="4"/>
<connect gate="G$1" pin="P0-7" pad="5"/>
<connect gate="G$1" pin="P0-8" pad="8"/>
<connect gate="G$1" pin="P0-9" pad="9"/>
<connect gate="G$1" pin="P1-0" pad="30"/>
<connect gate="G$1" pin="P1-1" pad="31"/>
<connect gate="G$1" pin="P1-10" pad="42"/>
<connect gate="G$1" pin="P1-11" pad="43"/>
<connect gate="G$1" pin="P1-12" pad="44"/>
<connect gate="G$1" pin="P1-13" pad="45"/>
<connect gate="G$1" pin="P1-14" pad="46"/>
<connect gate="G$1" pin="P1-15" pad="47"/>
<connect gate="G$1" pin="P1-2" pad="32"/>
<connect gate="G$1" pin="P1-3" pad="33"/>
<connect gate="G$1" pin="P1-4" pad="34"/>
<connect gate="G$1" pin="P1-5" pad="35"/>
<connect gate="G$1" pin="P1-6" pad="36"/>
<connect gate="G$1" pin="P1-7" pad="37"/>
<connect gate="G$1" pin="P1-8" pad="40"/>
<connect gate="G$1" pin="P1-9" pad="41"/>
<connect gate="G$1" pin="P2-0" pad="62"/>
<connect gate="G$1" pin="P2-1" pad="63"/>
<connect gate="G$1" pin="P2-10" pad="72"/>
<connect gate="G$1" pin="P2-11" pad="73"/>
<connect gate="G$1" pin="P2-12" pad="74"/>
<connect gate="G$1" pin="P2-13" pad="75"/>
<connect gate="G$1" pin="P2-14" pad="76"/>
<connect gate="G$1" pin="P2-15" pad="77"/>
<connect gate="G$1" pin="P2-2" pad="64"/>
<connect gate="G$1" pin="P2-3" pad="65"/>
<connect gate="G$1" pin="P2-4" pad="66"/>
<connect gate="G$1" pin="P2-5" pad="67"/>
<connect gate="G$1" pin="P2-6" pad="68"/>
<connect gate="G$1" pin="P2-7" pad="69"/>
<connect gate="G$1" pin="P2-8" pad="70"/>
<connect gate="G$1" pin="P2-9" pad="71"/>
<connect gate="G$1" pin="P3-0" pad="80"/>
<connect gate="G$1" pin="P3-1" pad="81"/>
<connect gate="G$1" pin="P3-10" pad="90"/>
<connect gate="G$1" pin="P3-11" pad="91"/>
<connect gate="G$1" pin="P3-12" pad="92"/>
<connect gate="G$1" pin="P3-13" pad="95"/>
<connect gate="G$1" pin="P3-14" pad="96"/>
<connect gate="G$1" pin="P3-15" pad="97"/>
<connect gate="G$1" pin="P3-2" pad="82"/>
<connect gate="G$1" pin="P3-3" pad="83"/>
<connect gate="G$1" pin="P3-4" pad="84"/>
<connect gate="G$1" pin="P3-5" pad="85"/>
<connect gate="G$1" pin="P3-6" pad="86"/>
<connect gate="G$1" pin="P3-7" pad="87"/>
<connect gate="G$1" pin="P3-8" pad="88"/>
<connect gate="G$1" pin="P3-9" pad="89"/>
<connect gate="G$1" pin="P4-0" pad="16"/>
<connect gate="G$1" pin="P4-1" pad="17"/>
<connect gate="G$1" pin="P5-0" pad="48"/>
<connect gate="G$1" pin="P5-1" pad="49"/>
<connect gate="G$1" pin="P5-2" pad="50"/>
<connect gate="G$1" pin="P5-3" pad="51"/>
<connect gate="G$1" pin="P5-4" pad="52"/>
<connect gate="G$1" pin="P5-5" pad="53"/>
<connect gate="G$1" pin="P5-6" pad="56"/>
<connect gate="G$1" pin="P5-7" pad="57"/>
<connect gate="G$1" pin="P5-8" pad="58"/>
<connect gate="G$1" pin="P5-9" pad="59"/>
<connect gate="G$1" pin="VAGND" pad="55"/>
<connect gate="G$1" pin="VAREF" pad="54"/>
<connect gate="G$1" pin="XTAL1" pad="20"/>
<connect gate="G$1" pin="XTAL2" pad="19"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="18"/>
<connect gate="P" pin="VCC@3" pad="38"/>
<connect gate="P" pin="VCC@4" pad="61"/>
<connect gate="P" pin="VCC@5" pad="79"/>
<connect gate="P" pin="VCC@6" pad="93"/>
<connect gate="P" pin="VSS@1" pad="6"/>
<connect gate="P" pin="VSS@2" pad="21"/>
<connect gate="P" pin="VSS@3" pad="39"/>
<connect gate="P" pin="VSS@4" pad="60"/>
<connect gate="P" pin="VSS@5" pad="78"/>
<connect gate="P" pin="VSS@6" pad="94"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C165-RM" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C165"/>
<gate name="P" symbol="6_VCCVSS"/>
</gates>
<devices>
<device name="" package="MQFP100">
<connects>
<connect gate="G$1" pin="!EA" pad="39"/>
<connect gate="G$1" pin="!NMI" pad="83"/>
<connect gate="G$1" pin="!RD" pad="35"/>
<connect gate="G$1" pin="!READY" pad="37"/>
<connect gate="G$1" pin="!RSTIN" pad="81"/>
<connect gate="G$1" pin="!RSTOUT" pad="82"/>
<connect gate="G$1" pin="!WR!/!WRL" pad="36"/>
<connect gate="G$1" pin="ALE" pad="38"/>
<connect gate="G$1" pin="P0H-0" pad="53"/>
<connect gate="G$1" pin="P0H-1" pad="54"/>
<connect gate="G$1" pin="P0H-2" pad="55"/>
<connect gate="G$1" pin="P0H-3" pad="56"/>
<connect gate="G$1" pin="P0H-4" pad="57"/>
<connect gate="G$1" pin="P0H-5" pad="58"/>
<connect gate="G$1" pin="P0H-6" pad="59"/>
<connect gate="G$1" pin="P0H-7" pad="60"/>
<connect gate="G$1" pin="P0L-0" pad="43"/>
<connect gate="G$1" pin="P0L-1" pad="44"/>
<connect gate="G$1" pin="P0L-2" pad="45"/>
<connect gate="G$1" pin="P0L-3" pad="46"/>
<connect gate="G$1" pin="P0L-4" pad="47"/>
<connect gate="G$1" pin="P0L-5" pad="48"/>
<connect gate="G$1" pin="P0L-6" pad="49"/>
<connect gate="G$1" pin="P0L-7" pad="50"/>
<connect gate="G$1" pin="P1H-0" pad="69"/>
<connect gate="G$1" pin="P1H-1" pad="70"/>
<connect gate="G$1" pin="P1H-2" pad="73"/>
<connect gate="G$1" pin="P1H-3" pad="74"/>
<connect gate="G$1" pin="P1H-4" pad="75"/>
<connect gate="G$1" pin="P1H-5" pad="76"/>
<connect gate="G$1" pin="P1H-6" pad="77"/>
<connect gate="G$1" pin="P1H-7" pad="78"/>
<connect gate="G$1" pin="P1L-0" pad="61"/>
<connect gate="G$1" pin="P1L-1" pad="62"/>
<connect gate="G$1" pin="P1L-2" pad="63"/>
<connect gate="G$1" pin="P1L-3" pad="64"/>
<connect gate="G$1" pin="P1L-4" pad="65"/>
<connect gate="G$1" pin="P1L-5" pad="66"/>
<connect gate="G$1" pin="P1L-6" pad="67"/>
<connect gate="G$1" pin="P1L-7" pad="68"/>
<connect gate="G$1" pin="P2-10" pad="94"/>
<connect gate="G$1" pin="P2-11" pad="95"/>
<connect gate="G$1" pin="P2-12" pad="96"/>
<connect gate="G$1" pin="P2-13" pad="97"/>
<connect gate="G$1" pin="P2-14" pad="98"/>
<connect gate="G$1" pin="P2-15" pad="99"/>
<connect gate="G$1" pin="P2-8" pad="92"/>
<connect gate="G$1" pin="P2-9" pad="93"/>
<connect gate="G$1" pin="P3-0" pad="10"/>
<connect gate="G$1" pin="P3-1" pad="11"/>
<connect gate="G$1" pin="P3-10" pad="20"/>
<connect gate="G$1" pin="P3-11" pad="21"/>
<connect gate="G$1" pin="P3-12" pad="22"/>
<connect gate="G$1" pin="P3-13" pad="23"/>
<connect gate="G$1" pin="P3-15" pad="24"/>
<connect gate="G$1" pin="P3-2" pad="12"/>
<connect gate="G$1" pin="P3-3" pad="13"/>
<connect gate="G$1" pin="P3-4" pad="14"/>
<connect gate="G$1" pin="P3-5" pad="15"/>
<connect gate="G$1" pin="P3-6" pad="16"/>
<connect gate="G$1" pin="P3-7" pad="17"/>
<connect gate="G$1" pin="P3-8" pad="18"/>
<connect gate="G$1" pin="P3-9" pad="19"/>
<connect gate="G$1" pin="P4-0" pad="25"/>
<connect gate="G$1" pin="P4-1" pad="26"/>
<connect gate="G$1" pin="P4-2" pad="27"/>
<connect gate="G$1" pin="P4-3" pad="28"/>
<connect gate="G$1" pin="P4-4" pad="31"/>
<connect gate="G$1" pin="P4-5" pad="32"/>
<connect gate="G$1" pin="P4-6" pad="33"/>
<connect gate="G$1" pin="P4-7" pad="34"/>
<connect gate="G$1" pin="P5-10" pad="100"/>
<connect gate="G$1" pin="P5-11" pad="1"/>
<connect gate="G$1" pin="P5-12" pad="2"/>
<connect gate="G$1" pin="P5-13" pad="3"/>
<connect gate="G$1" pin="P5-14" pad="4"/>
<connect gate="G$1" pin="P5-15" pad="5"/>
<connect gate="G$1" pin="P6-0" pad="84"/>
<connect gate="G$1" pin="P6-1" pad="85"/>
<connect gate="G$1" pin="P6-2" pad="86"/>
<connect gate="G$1" pin="P6-3" pad="87"/>
<connect gate="G$1" pin="P6-4" pad="88"/>
<connect gate="G$1" pin="P6-5" pad="89"/>
<connect gate="G$1" pin="P6-6" pad="90"/>
<connect gate="G$1" pin="P6-7" pad="91"/>
<connect gate="G$1" pin="VPP" pad="42"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
<connect gate="P" pin="VCC@1" pad="9"/>
<connect gate="P" pin="VCC@2" pad="30"/>
<connect gate="P" pin="VCC@3" pad="40"/>
<connect gate="P" pin="VCC@4" pad="51"/>
<connect gate="P" pin="VCC@5" pad="71"/>
<connect gate="P" pin="VCC@6" pad="80"/>
<connect gate="P" pin="VSS@1" pad="6"/>
<connect gate="P" pin="VSS@2" pad="29"/>
<connect gate="P" pin="VSS@3" pad="41"/>
<connect gate="P" pin="VSS@4" pad="52"/>
<connect gate="P" pin="VSS@5" pad="72"/>
<connect gate="P" pin="VSS@6" pad="79"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C165-RF" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C165"/>
<gate name="P" symbol="6_VCCVSS"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G$1" pin="!EA" pad="37"/>
<connect gate="G$1" pin="!NMI" pad="81"/>
<connect gate="G$1" pin="!RD" pad="33"/>
<connect gate="G$1" pin="!READY" pad="35"/>
<connect gate="G$1" pin="!RSTIN" pad="79"/>
<connect gate="G$1" pin="!RSTOUT" pad="80"/>
<connect gate="G$1" pin="!WR!/!WRL" pad="34"/>
<connect gate="G$1" pin="ALE" pad="36"/>
<connect gate="G$1" pin="P0H-0" pad="51"/>
<connect gate="G$1" pin="P0H-1" pad="52"/>
<connect gate="G$1" pin="P0H-2" pad="53"/>
<connect gate="G$1" pin="P0H-3" pad="54"/>
<connect gate="G$1" pin="P0H-4" pad="55"/>
<connect gate="G$1" pin="P0H-5" pad="56"/>
<connect gate="G$1" pin="P0H-6" pad="57"/>
<connect gate="G$1" pin="P0H-7" pad="58"/>
<connect gate="G$1" pin="P0L-0" pad="41"/>
<connect gate="G$1" pin="P0L-1" pad="42"/>
<connect gate="G$1" pin="P0L-2" pad="43"/>
<connect gate="G$1" pin="P0L-3" pad="44"/>
<connect gate="G$1" pin="P0L-4" pad="45"/>
<connect gate="G$1" pin="P0L-5" pad="46"/>
<connect gate="G$1" pin="P0L-6" pad="47"/>
<connect gate="G$1" pin="P0L-7" pad="48"/>
<connect gate="G$1" pin="P1H-0" pad="67"/>
<connect gate="G$1" pin="P1H-1" pad="68"/>
<connect gate="G$1" pin="P1H-2" pad="71"/>
<connect gate="G$1" pin="P1H-3" pad="72"/>
<connect gate="G$1" pin="P1H-4" pad="73"/>
<connect gate="G$1" pin="P1H-5" pad="74"/>
<connect gate="G$1" pin="P1H-6" pad="75"/>
<connect gate="G$1" pin="P1H-7" pad="76"/>
<connect gate="G$1" pin="P1L-0" pad="59"/>
<connect gate="G$1" pin="P1L-1" pad="60"/>
<connect gate="G$1" pin="P1L-2" pad="61"/>
<connect gate="G$1" pin="P1L-3" pad="62"/>
<connect gate="G$1" pin="P1L-4" pad="63"/>
<connect gate="G$1" pin="P1L-5" pad="64"/>
<connect gate="G$1" pin="P1L-6" pad="65"/>
<connect gate="G$1" pin="P1L-7" pad="66"/>
<connect gate="G$1" pin="P2-10" pad="92"/>
<connect gate="G$1" pin="P2-11" pad="93"/>
<connect gate="G$1" pin="P2-12" pad="94"/>
<connect gate="G$1" pin="P2-13" pad="95"/>
<connect gate="G$1" pin="P2-14" pad="96"/>
<connect gate="G$1" pin="P2-15" pad="97"/>
<connect gate="G$1" pin="P2-8" pad="90"/>
<connect gate="G$1" pin="P2-9" pad="91"/>
<connect gate="G$1" pin="P3-0" pad="8"/>
<connect gate="G$1" pin="P3-1" pad="9"/>
<connect gate="G$1" pin="P3-10" pad="18"/>
<connect gate="G$1" pin="P3-11" pad="19"/>
<connect gate="G$1" pin="P3-12" pad="20"/>
<connect gate="G$1" pin="P3-13" pad="21"/>
<connect gate="G$1" pin="P3-15" pad="22"/>
<connect gate="G$1" pin="P3-2" pad="10"/>
<connect gate="G$1" pin="P3-3" pad="11"/>
<connect gate="G$1" pin="P3-4" pad="12"/>
<connect gate="G$1" pin="P3-5" pad="13"/>
<connect gate="G$1" pin="P3-6" pad="14"/>
<connect gate="G$1" pin="P3-7" pad="15"/>
<connect gate="G$1" pin="P3-8" pad="16"/>
<connect gate="G$1" pin="P3-9" pad="17"/>
<connect gate="G$1" pin="P4-0" pad="23"/>
<connect gate="G$1" pin="P4-1" pad="24"/>
<connect gate="G$1" pin="P4-2" pad="25"/>
<connect gate="G$1" pin="P4-3" pad="26"/>
<connect gate="G$1" pin="P4-4" pad="29"/>
<connect gate="G$1" pin="P4-5" pad="30"/>
<connect gate="G$1" pin="P4-6" pad="31"/>
<connect gate="G$1" pin="P4-7" pad="32"/>
<connect gate="G$1" pin="P5-10" pad="98"/>
<connect gate="G$1" pin="P5-11" pad="99"/>
<connect gate="G$1" pin="P5-12" pad="100"/>
<connect gate="G$1" pin="P5-13" pad="1"/>
<connect gate="G$1" pin="P5-14" pad="2"/>
<connect gate="G$1" pin="P5-15" pad="3"/>
<connect gate="G$1" pin="P6-0" pad="82"/>
<connect gate="G$1" pin="P6-1" pad="83"/>
<connect gate="G$1" pin="P6-2" pad="84"/>
<connect gate="G$1" pin="P6-3" pad="85"/>
<connect gate="G$1" pin="P6-4" pad="86"/>
<connect gate="G$1" pin="P6-5" pad="87"/>
<connect gate="G$1" pin="P6-6" pad="88"/>
<connect gate="G$1" pin="P6-7" pad="89"/>
<connect gate="G$1" pin="VPP" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="6"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="28"/>
<connect gate="P" pin="VCC@3" pad="38"/>
<connect gate="P" pin="VCC@4" pad="49"/>
<connect gate="P" pin="VCC@5" pad="69"/>
<connect gate="P" pin="VCC@6" pad="78"/>
<connect gate="P" pin="VSS@1" pad="4"/>
<connect gate="P" pin="VSS@2" pad="27"/>
<connect gate="P" pin="VSS@3" pad="39"/>
<connect gate="P" pin="VSS@4" pad="50"/>
<connect gate="P" pin="VSS@5" pad="70"/>
<connect gate="P" pin="VSS@6" pad="77"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1472708"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C167-LM" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C167"/>
<gate name="P" symbol="10VCCVSS"/>
</gates>
<devices>
<device name="" package="MQFP144">
<connects>
<connect gate="G$1" pin="!EA" pad="99"/>
<connect gate="G$1" pin="!NMI" pad="142"/>
<connect gate="G$1" pin="!RD" pad="95"/>
<connect gate="G$1" pin="!READY" pad="97"/>
<connect gate="G$1" pin="!RSTIN" pad="140"/>
<connect gate="G$1" pin="!RSTOUT" pad="141"/>
<connect gate="G$1" pin="!WR!/!WRL" pad="96"/>
<connect gate="G$1" pin="ALE" pad="98"/>
<connect gate="G$1" pin="P0H-0" pad="108"/>
<connect gate="G$1" pin="P0H-1" pad="111"/>
<connect gate="G$1" pin="P0H-2" pad="112"/>
<connect gate="G$1" pin="P0H-3" pad="113"/>
<connect gate="G$1" pin="P0H-4" pad="114"/>
<connect gate="G$1" pin="P0H-5" pad="115"/>
<connect gate="G$1" pin="P0H-6" pad="116"/>
<connect gate="G$1" pin="P0H-7" pad="117"/>
<connect gate="G$1" pin="P0L-0" pad="100"/>
<connect gate="G$1" pin="P0L-1" pad="101"/>
<connect gate="G$1" pin="P0L-2" pad="102"/>
<connect gate="G$1" pin="P0L-3" pad="103"/>
<connect gate="G$1" pin="P0L-4" pad="104"/>
<connect gate="G$1" pin="P0L-5" pad="105"/>
<connect gate="G$1" pin="P0L-6" pad="106"/>
<connect gate="G$1" pin="P0L-7" pad="107"/>
<connect gate="G$1" pin="P1H-0" pad="128"/>
<connect gate="G$1" pin="P1H-1" pad="129"/>
<connect gate="G$1" pin="P1H-2" pad="130"/>
<connect gate="G$1" pin="P1H-3" pad="131"/>
<connect gate="G$1" pin="P1H-4" pad="132"/>
<connect gate="G$1" pin="P1H-5" pad="133"/>
<connect gate="G$1" pin="P1H-6" pad="134"/>
<connect gate="G$1" pin="P1H-7" pad="135"/>
<connect gate="G$1" pin="P1L-0" pad="118"/>
<connect gate="G$1" pin="P1L-1" pad="119"/>
<connect gate="G$1" pin="P1L-2" pad="120"/>
<connect gate="G$1" pin="P1L-3" pad="121"/>
<connect gate="G$1" pin="P1L-4" pad="122"/>
<connect gate="G$1" pin="P1L-5" pad="123"/>
<connect gate="G$1" pin="P1L-6" pad="124"/>
<connect gate="G$1" pin="P1L-7" pad="125"/>
<connect gate="G$1" pin="P2-0" pad="47"/>
<connect gate="G$1" pin="P2-1" pad="48"/>
<connect gate="G$1" pin="P2-10" pad="59"/>
<connect gate="G$1" pin="P2-11" pad="60"/>
<connect gate="G$1" pin="P2-12" pad="61"/>
<connect gate="G$1" pin="P2-13" pad="62"/>
<connect gate="G$1" pin="P2-14" pad="63"/>
<connect gate="G$1" pin="P2-15" pad="64"/>
<connect gate="G$1" pin="P2-2" pad="49"/>
<connect gate="G$1" pin="P2-3" pad="50"/>
<connect gate="G$1" pin="P2-4" pad="51"/>
<connect gate="G$1" pin="P2-5" pad="52"/>
<connect gate="G$1" pin="P2-6" pad="53"/>
<connect gate="G$1" pin="P2-7" pad="54"/>
<connect gate="G$1" pin="P2-8" pad="57"/>
<connect gate="G$1" pin="P2-9" pad="58"/>
<connect gate="G$1" pin="P3-0" pad="65"/>
<connect gate="G$1" pin="P3-1" pad="66"/>
<connect gate="G$1" pin="P3-10" pad="77"/>
<connect gate="G$1" pin="P3-11" pad="78"/>
<connect gate="G$1" pin="P3-12" pad="79"/>
<connect gate="G$1" pin="P3-13" pad="80"/>
<connect gate="G$1" pin="P3-15" pad="81"/>
<connect gate="G$1" pin="P3-2" pad="67"/>
<connect gate="G$1" pin="P3-3" pad="68"/>
<connect gate="G$1" pin="P3-4" pad="69"/>
<connect gate="G$1" pin="P3-5" pad="70"/>
<connect gate="G$1" pin="P3-6" pad="73"/>
<connect gate="G$1" pin="P3-7" pad="74"/>
<connect gate="G$1" pin="P3-8" pad="75"/>
<connect gate="G$1" pin="P3-9" pad="76"/>
<connect gate="G$1" pin="P4-0" pad="85"/>
<connect gate="G$1" pin="P4-1" pad="86"/>
<connect gate="G$1" pin="P4-2" pad="87"/>
<connect gate="G$1" pin="P4-3" pad="88"/>
<connect gate="G$1" pin="P4-4" pad="89"/>
<connect gate="G$1" pin="P4-5" pad="90"/>
<connect gate="G$1" pin="P4-6" pad="91"/>
<connect gate="G$1" pin="P4-7" pad="92"/>
<connect gate="G$1" pin="P5-0" pad="27"/>
<connect gate="G$1" pin="P5-1" pad="28"/>
<connect gate="G$1" pin="P5-10" pad="39"/>
<connect gate="G$1" pin="P5-11" pad="40"/>
<connect gate="G$1" pin="P5-12" pad="41"/>
<connect gate="G$1" pin="P5-13" pad="42"/>
<connect gate="G$1" pin="P5-14" pad="43"/>
<connect gate="G$1" pin="P5-15" pad="44"/>
<connect gate="G$1" pin="P5-2" pad="29"/>
<connect gate="G$1" pin="P5-3" pad="30"/>
<connect gate="G$1" pin="P5-4" pad="31"/>
<connect gate="G$1" pin="P5-5" pad="32"/>
<connect gate="G$1" pin="P5-6" pad="33"/>
<connect gate="G$1" pin="P5-7" pad="34"/>
<connect gate="G$1" pin="P5-8" pad="35"/>
<connect gate="G$1" pin="P5-9" pad="36"/>
<connect gate="G$1" pin="P6-0" pad="1"/>
<connect gate="G$1" pin="P6-1" pad="2"/>
<connect gate="G$1" pin="P6-2" pad="3"/>
<connect gate="G$1" pin="P6-3" pad="4"/>
<connect gate="G$1" pin="P6-4" pad="5"/>
<connect gate="G$1" pin="P6-5" pad="6"/>
<connect gate="G$1" pin="P6-6" pad="7"/>
<connect gate="G$1" pin="P6-7" pad="8"/>
<connect gate="G$1" pin="P7-0" pad="19"/>
<connect gate="G$1" pin="P7-1" pad="20"/>
<connect gate="G$1" pin="P7-2" pad="21"/>
<connect gate="G$1" pin="P7-3" pad="22"/>
<connect gate="G$1" pin="P7-4" pad="23"/>
<connect gate="G$1" pin="P7-5" pad="24"/>
<connect gate="G$1" pin="P7-6" pad="25"/>
<connect gate="G$1" pin="P7-7" pad="26"/>
<connect gate="G$1" pin="P8-0" pad="9"/>
<connect gate="G$1" pin="P8-1" pad="10"/>
<connect gate="G$1" pin="P8-2" pad="11"/>
<connect gate="G$1" pin="P8-3" pad="12"/>
<connect gate="G$1" pin="P8-4" pad="13"/>
<connect gate="G$1" pin="P8-5" pad="14"/>
<connect gate="G$1" pin="P8-6" pad="15"/>
<connect gate="G$1" pin="P8-7" pad="16"/>
<connect gate="G$1" pin="VAGND" pad="38"/>
<connect gate="G$1" pin="VAREF" pad="37"/>
<connect gate="G$1" pin="VPP" pad="84"/>
<connect gate="G$1" pin="XTAL1" pad="138"/>
<connect gate="G$1" pin="XTAL2" pad="137"/>
<connect gate="P" pin="VCC@1" pad="17"/>
<connect gate="P" pin="VCC@10" pad="144"/>
<connect gate="P" pin="VCC@2" pad="46"/>
<connect gate="P" pin="VCC@3" pad="56"/>
<connect gate="P" pin="VCC@4" pad="72"/>
<connect gate="P" pin="VCC@5" pad="82"/>
<connect gate="P" pin="VCC@6" pad="93"/>
<connect gate="P" pin="VCC@7" pad="109"/>
<connect gate="P" pin="VCC@8" pad="126"/>
<connect gate="P" pin="VCC@9" pad="136"/>
<connect gate="P" pin="VSS@1" pad="18"/>
<connect gate="P" pin="VSS@10" pad="143"/>
<connect gate="P" pin="VSS@2" pad="45"/>
<connect gate="P" pin="VSS@3" pad="55"/>
<connect gate="P" pin="VSS@4" pad="71"/>
<connect gate="P" pin="VSS@5" pad="83"/>
<connect gate="P" pin="VSS@6" pad="94"/>
<connect gate="P" pin="VSS@7" pad="110"/>
<connect gate="P" pin="VSS@8" pad="127"/>
<connect gate="P" pin="VSS@9" pad="139"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1472745"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80186" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80186"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!BHE!/S7" pad="5"/>
<connect gate="G$1" pin="!DEN" pad="48"/>
<connect gate="G$1" pin="!LCS" pad="42"/>
<connect gate="G$1" pin="!LOCK" pad="57"/>
<connect gate="G$1" pin="!MCS0" pad="47"/>
<connect gate="G$1" pin="!MCS1" pad="46"/>
<connect gate="G$1" pin="!MCS2" pad="45"/>
<connect gate="G$1" pin="!MCS3" pad="44"/>
<connect gate="G$1" pin="!PCS0" pad="34"/>
<connect gate="G$1" pin="!PCS1" pad="36"/>
<connect gate="G$1" pin="!PCS2" pad="37"/>
<connect gate="G$1" pin="!PCS3" pad="38"/>
<connect gate="G$1" pin="!PCS4" pad="39"/>
<connect gate="G$1" pin="!PCS5!/A1" pad="40"/>
<connect gate="G$1" pin="!PCS6!/A2" pad="41"/>
<connect gate="G$1" pin="!RD!/!QSMD" pad="3"/>
<connect gate="G$1" pin="!RES" pad="33"/>
<connect gate="G$1" pin="!S0" pad="61"/>
<connect gate="G$1" pin="!S1" pad="62"/>
<connect gate="G$1" pin="!S2" pad="63"/>
<connect gate="G$1" pin="!TEST" pad="56"/>
<connect gate="G$1" pin="!UCS" pad="43"/>
<connect gate="G$1" pin="!WR!/QS1" pad="4"/>
<connect gate="G$1" pin="A16/S3" pad="9"/>
<connect gate="G$1" pin="A17/S4" pad="8"/>
<connect gate="G$1" pin="A18/S5" pad="7"/>
<connect gate="G$1" pin="A19/S6" pad="6"/>
<connect gate="G$1" pin="AD0" pad="26"/>
<connect gate="G$1" pin="AD1" pad="24"/>
<connect gate="G$1" pin="AD10" pad="21"/>
<connect gate="G$1" pin="AD11" pad="19"/>
<connect gate="G$1" pin="AD12" pad="16"/>
<connect gate="G$1" pin="AD13" pad="14"/>
<connect gate="G$1" pin="AD14" pad="12"/>
<connect gate="G$1" pin="AD15" pad="10"/>
<connect gate="G$1" pin="AD2" pad="22"/>
<connect gate="G$1" pin="AD3" pad="20"/>
<connect gate="G$1" pin="AD4" pad="17"/>
<connect gate="G$1" pin="AD5" pad="15"/>
<connect gate="G$1" pin="AD6" pad="13"/>
<connect gate="G$1" pin="AD7" pad="11"/>
<connect gate="G$1" pin="AD8" pad="25"/>
<connect gate="G$1" pin="AD9" pad="23"/>
<connect gate="G$1" pin="ALE/QS0" pad="2"/>
<connect gate="G$1" pin="ARDY" pad="64"/>
<connect gate="G$1" pin="CLKOUT" pad="65"/>
<connect gate="G$1" pin="DRQ0" pad="27"/>
<connect gate="G$1" pin="DRQ1" pad="28"/>
<connect gate="G$1" pin="DT/!R" pad="49"/>
<connect gate="G$1" pin="HLDA" pad="60"/>
<connect gate="G$1" pin="HOLD" pad="59"/>
<connect gate="G$1" pin="INT0" pad="54"/>
<connect gate="G$1" pin="INT1" pad="53"/>
<connect gate="G$1" pin="INT2/INTA0" pad="51"/>
<connect gate="G$1" pin="INT3/INTA1" pad="50"/>
<connect gate="G$1" pin="NMI" pad="55"/>
<connect gate="G$1" pin="RESET" pad="66"/>
<connect gate="G$1" pin="SRDY" pad="58"/>
<connect gate="G$1" pin="TMRIN0" pad="29"/>
<connect gate="G$1" pin="TMRIN1" pad="30"/>
<connect gate="G$1" pin="TMROUT0" pad="31"/>
<connect gate="G$1" pin="TMROUT1" pad="32"/>
<connect gate="G$1" pin="X1" pad="68"/>
<connect gate="G$1" pin="X2" pad="67"/>
<connect gate="P" pin="GND@1" pad="35"/>
<connect gate="P" pin="GND@2" pad="1"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="52"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C503" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C503"/>
<gate name="P" symbol="1VCC2VSS"/>
</gates>
<devices>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="!EA" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="33"/>
<connect gate="G$1" pin="ALE" pad="34"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="P0-0" pad="43"/>
<connect gate="G$1" pin="P0-1" pad="42"/>
<connect gate="G$1" pin="P0-2" pad="41"/>
<connect gate="G$1" pin="P0-3" pad="40"/>
<connect gate="G$1" pin="P0-4" pad="39"/>
<connect gate="G$1" pin="P0-5" pad="38"/>
<connect gate="G$1" pin="P0-6" pad="37"/>
<connect gate="G$1" pin="P0-7" pad="36"/>
<connect gate="G$1" pin="P1-0" pad="5"/>
<connect gate="G$1" pin="P1-1" pad="6"/>
<connect gate="G$1" pin="P1-2" pad="7"/>
<connect gate="G$1" pin="P1-3" pad="8"/>
<connect gate="G$1" pin="P1-4" pad="9"/>
<connect gate="G$1" pin="P1-5" pad="10"/>
<connect gate="G$1" pin="P1-6" pad="11"/>
<connect gate="G$1" pin="P1-7" pad="12"/>
<connect gate="G$1" pin="P2-0" pad="25"/>
<connect gate="G$1" pin="P2-1" pad="26"/>
<connect gate="G$1" pin="P2-2" pad="27"/>
<connect gate="G$1" pin="P2-3" pad="28"/>
<connect gate="G$1" pin="P2-4" pad="29"/>
<connect gate="G$1" pin="P2-5" pad="30"/>
<connect gate="G$1" pin="P2-6" pad="31"/>
<connect gate="G$1" pin="P2-7" pad="32"/>
<connect gate="G$1" pin="P3-0" pad="14"/>
<connect gate="G$1" pin="P3-1" pad="15"/>
<connect gate="G$1" pin="P3-2" pad="16"/>
<connect gate="G$1" pin="P3-3" pad="17"/>
<connect gate="G$1" pin="P3-4" pad="18"/>
<connect gate="G$1" pin="P3-5" pad="19"/>
<connect gate="G$1" pin="P3-6" pad="20"/>
<connect gate="G$1" pin="P3-7" pad="21"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="G$1" pin="VAGND" pad="3"/>
<connect gate="G$1" pin="VAREF" pad="2"/>
<connect gate="G$1" pin="XTAL1" pad="23"/>
<connect gate="G$1" pin="XTAL2" pad="22"/>
<connect gate="P" pin="VCC" pad="44"/>
<connect gate="P" pin="VSS" pad="24"/>
<connect gate="P" pin="VSS@1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C517-N" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C517-N"/>
<gate name="P" symbol="2VCC3VSS"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="G$1" pin="!EA" pad="51"/>
<connect gate="G$1" pin="!PE!/SWD" pad="4"/>
<connect gate="G$1" pin="!PSEN" pad="49"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="!RO" pad="82"/>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="OWE" pad="69"/>
<connect gate="G$1" pin="P0-0" pad="52"/>
<connect gate="G$1" pin="P0-1" pad="53"/>
<connect gate="G$1" pin="P0-2" pad="54"/>
<connect gate="G$1" pin="P0-3" pad="55"/>
<connect gate="G$1" pin="P0-4" pad="56"/>
<connect gate="G$1" pin="P0-5" pad="57"/>
<connect gate="G$1" pin="P0-6" pad="58"/>
<connect gate="G$1" pin="P0-7" pad="59"/>
<connect gate="G$1" pin="P1-0" pad="36"/>
<connect gate="G$1" pin="P1-1" pad="35"/>
<connect gate="G$1" pin="P1-2" pad="34"/>
<connect gate="G$1" pin="P1-3" pad="33"/>
<connect gate="G$1" pin="P1-4" pad="32"/>
<connect gate="G$1" pin="P1-5" pad="31"/>
<connect gate="G$1" pin="P1-6" pad="30"/>
<connect gate="G$1" pin="P1-7" pad="29"/>
<connect gate="G$1" pin="P2-0" pad="41"/>
<connect gate="G$1" pin="P2-1" pad="42"/>
<connect gate="G$1" pin="P2-2" pad="43"/>
<connect gate="G$1" pin="P2-3" pad="44"/>
<connect gate="G$1" pin="P2-4" pad="45"/>
<connect gate="G$1" pin="P2-5" pad="46"/>
<connect gate="G$1" pin="P2-6" pad="47"/>
<connect gate="G$1" pin="P2-7" pad="48"/>
<connect gate="G$1" pin="P3-0" pad="21"/>
<connect gate="G$1" pin="P3-1" pad="22"/>
<connect gate="G$1" pin="P3-2" pad="23"/>
<connect gate="G$1" pin="P3-3" pad="24"/>
<connect gate="G$1" pin="P3-4" pad="25"/>
<connect gate="G$1" pin="P3-5" pad="26"/>
<connect gate="G$1" pin="P3-6" pad="27"/>
<connect gate="G$1" pin="P3-7" pad="28"/>
<connect gate="G$1" pin="P4-0" pad="1"/>
<connect gate="G$1" pin="P4-1" pad="2"/>
<connect gate="G$1" pin="P4-2" pad="3"/>
<connect gate="G$1" pin="P4-3" pad="5"/>
<connect gate="G$1" pin="P4-4" pad="6"/>
<connect gate="G$1" pin="P4-5" pad="7"/>
<connect gate="G$1" pin="P4-6" pad="8"/>
<connect gate="G$1" pin="P4-7" pad="9"/>
<connect gate="G$1" pin="P5-0" pad="68"/>
<connect gate="G$1" pin="P5-1" pad="67"/>
<connect gate="G$1" pin="P5-2" pad="66"/>
<connect gate="G$1" pin="P5-3" pad="65"/>
<connect gate="G$1" pin="P5-4" pad="64"/>
<connect gate="G$1" pin="P5-5" pad="63"/>
<connect gate="G$1" pin="P5-6" pad="62"/>
<connect gate="G$1" pin="P5-7" pad="61"/>
<connect gate="G$1" pin="P6-0" pad="70"/>
<connect gate="G$1" pin="P6-1" pad="71"/>
<connect gate="G$1" pin="P6-2" pad="72"/>
<connect gate="G$1" pin="P6-3" pad="73"/>
<connect gate="G$1" pin="P6-4" pad="74"/>
<connect gate="G$1" pin="P6-5" pad="75"/>
<connect gate="G$1" pin="P6-6" pad="76"/>
<connect gate="G$1" pin="P6-7" pad="77"/>
<connect gate="G$1" pin="P7-0" pad="20"/>
<connect gate="G$1" pin="P7-1" pad="19"/>
<connect gate="G$1" pin="P7-2" pad="18"/>
<connect gate="G$1" pin="P7-3" pad="17"/>
<connect gate="G$1" pin="P7-4" pad="16"/>
<connect gate="G$1" pin="P7-5" pad="15"/>
<connect gate="G$1" pin="P7-6" pad="14"/>
<connect gate="G$1" pin="P7-7" pad="13"/>
<connect gate="G$1" pin="P8-0" pad="78"/>
<connect gate="G$1" pin="P8-1" pad="79"/>
<connect gate="G$1" pin="P8-2" pad="80"/>
<connect gate="G$1" pin="P8-3" pad="81"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="VCC@1" pad="38"/>
<connect gate="P" pin="VCC@2" pad="84"/>
<connect gate="P" pin="VSS@1" pad="37"/>
<connect gate="P" pin="VSS@2" pad="60"/>
<connect gate="P" pin="VSS@3" pad="83"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SOC" package="PLCC84SOCK">
<connects>
<connect gate="G$1" pin="!EA" pad="51"/>
<connect gate="G$1" pin="!PE!/SWD" pad="4"/>
<connect gate="G$1" pin="!PSEN" pad="49"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="!RO" pad="82"/>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="OWE" pad="69"/>
<connect gate="G$1" pin="P0-0" pad="52"/>
<connect gate="G$1" pin="P0-1" pad="53"/>
<connect gate="G$1" pin="P0-2" pad="54"/>
<connect gate="G$1" pin="P0-3" pad="55"/>
<connect gate="G$1" pin="P0-4" pad="56"/>
<connect gate="G$1" pin="P0-5" pad="57"/>
<connect gate="G$1" pin="P0-6" pad="58"/>
<connect gate="G$1" pin="P0-7" pad="59"/>
<connect gate="G$1" pin="P1-0" pad="36"/>
<connect gate="G$1" pin="P1-1" pad="35"/>
<connect gate="G$1" pin="P1-2" pad="34"/>
<connect gate="G$1" pin="P1-3" pad="33"/>
<connect gate="G$1" pin="P1-4" pad="32"/>
<connect gate="G$1" pin="P1-5" pad="31"/>
<connect gate="G$1" pin="P1-6" pad="30"/>
<connect gate="G$1" pin="P1-7" pad="29"/>
<connect gate="G$1" pin="P2-0" pad="41"/>
<connect gate="G$1" pin="P2-1" pad="42"/>
<connect gate="G$1" pin="P2-2" pad="43"/>
<connect gate="G$1" pin="P2-3" pad="44"/>
<connect gate="G$1" pin="P2-4" pad="45"/>
<connect gate="G$1" pin="P2-5" pad="46"/>
<connect gate="G$1" pin="P2-6" pad="47"/>
<connect gate="G$1" pin="P2-7" pad="48"/>
<connect gate="G$1" pin="P3-0" pad="21"/>
<connect gate="G$1" pin="P3-1" pad="22"/>
<connect gate="G$1" pin="P3-2" pad="23"/>
<connect gate="G$1" pin="P3-3" pad="24"/>
<connect gate="G$1" pin="P3-4" pad="25"/>
<connect gate="G$1" pin="P3-5" pad="26"/>
<connect gate="G$1" pin="P3-6" pad="27"/>
<connect gate="G$1" pin="P3-7" pad="28"/>
<connect gate="G$1" pin="P4-0" pad="1"/>
<connect gate="G$1" pin="P4-1" pad="2"/>
<connect gate="G$1" pin="P4-2" pad="3"/>
<connect gate="G$1" pin="P4-3" pad="5"/>
<connect gate="G$1" pin="P4-4" pad="6"/>
<connect gate="G$1" pin="P4-5" pad="7"/>
<connect gate="G$1" pin="P4-6" pad="8"/>
<connect gate="G$1" pin="P4-7" pad="9"/>
<connect gate="G$1" pin="P5-0" pad="68"/>
<connect gate="G$1" pin="P5-1" pad="67"/>
<connect gate="G$1" pin="P5-2" pad="66"/>
<connect gate="G$1" pin="P5-3" pad="65"/>
<connect gate="G$1" pin="P5-4" pad="64"/>
<connect gate="G$1" pin="P5-5" pad="63"/>
<connect gate="G$1" pin="P5-6" pad="62"/>
<connect gate="G$1" pin="P5-7" pad="61"/>
<connect gate="G$1" pin="P6-0" pad="70"/>
<connect gate="G$1" pin="P6-1" pad="71"/>
<connect gate="G$1" pin="P6-2" pad="72"/>
<connect gate="G$1" pin="P6-3" pad="73"/>
<connect gate="G$1" pin="P6-4" pad="74"/>
<connect gate="G$1" pin="P6-5" pad="75"/>
<connect gate="G$1" pin="P6-6" pad="76"/>
<connect gate="G$1" pin="P6-7" pad="77"/>
<connect gate="G$1" pin="P7-0" pad="20"/>
<connect gate="G$1" pin="P7-1" pad="19"/>
<connect gate="G$1" pin="P7-2" pad="18"/>
<connect gate="G$1" pin="P7-3" pad="17"/>
<connect gate="G$1" pin="P7-4" pad="16"/>
<connect gate="G$1" pin="P7-5" pad="15"/>
<connect gate="G$1" pin="P7-6" pad="14"/>
<connect gate="G$1" pin="P7-7" pad="13"/>
<connect gate="G$1" pin="P8-0" pad="78"/>
<connect gate="G$1" pin="P8-1" pad="79"/>
<connect gate="G$1" pin="P8-2" pad="80"/>
<connect gate="G$1" pin="P8-3" pad="81"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="VCC@1" pad="38"/>
<connect gate="P" pin="VCC@2" pad="84"/>
<connect gate="P" pin="VSS@1" pad="37"/>
<connect gate="P" pin="VSS@2" pad="60"/>
<connect gate="P" pin="VSS@3" pad="83"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C517-M" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C517-M"/>
<gate name="P" symbol="2VCC2VSS"/>
</gates>
<devices>
<device name="" package="MQFP100">
<connects>
<connect gate="G$1" pin="!EA" pad="24"/>
<connect gate="G$1" pin="!PE!/SWD" pad="67"/>
<connect gate="G$1" pin="!PSEN" pad="22"/>
<connect gate="G$1" pin="!RESET" pad="73"/>
<connect gate="G$1" pin="!RO" pad="61"/>
<connect gate="G$1" pin="ALE" pad="23"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@10" pad="52"/>
<connect gate="G$1" pin="NC@11" pad="53"/>
<connect gate="G$1" pin="NC@12" pad="74"/>
<connect gate="G$1" pin="NC@13" pad="75"/>
<connect gate="G$1" pin="NC@14" pad="76"/>
<connect gate="G$1" pin="NC@15" pad="77"/>
<connect gate="G$1" pin="NC@16" pad="88"/>
<connect gate="G$1" pin="NC@17" pad="89"/>
<connect gate="G$1" pin="NC@2" pad="3"/>
<connect gate="G$1" pin="NC@3" pad="4"/>
<connect gate="G$1" pin="NC@4" pad="5"/>
<connect gate="G$1" pin="NC@5" pad="25"/>
<connect gate="G$1" pin="NC@6" pad="28"/>
<connect gate="G$1" pin="NC@7" pad="29"/>
<connect gate="G$1" pin="NC@8" pad="36"/>
<connect gate="G$1" pin="NC@9" pad="51"/>
<connect gate="G$1" pin="OWE" pad="45"/>
<connect gate="G$1" pin="P0-0" pad="26"/>
<connect gate="G$1" pin="P0-1" pad="27"/>
<connect gate="G$1" pin="P0-2" pad="30"/>
<connect gate="G$1" pin="P0-3" pad="31"/>
<connect gate="G$1" pin="P0-4" pad="32"/>
<connect gate="G$1" pin="P0-5" pad="33"/>
<connect gate="G$1" pin="P0-6" pad="34"/>
<connect gate="G$1" pin="P0-7" pad="35"/>
<connect gate="G$1" pin="P1-0" pad="9"/>
<connect gate="G$1" pin="P1-1" pad="8"/>
<connect gate="G$1" pin="P1-2" pad="7"/>
<connect gate="G$1" pin="P1-3" pad="6"/>
<connect gate="G$1" pin="P1-4" pad="1"/>
<connect gate="G$1" pin="P1-5" pad="100"/>
<connect gate="G$1" pin="P1-6" pad="99"/>
<connect gate="G$1" pin="P1-7" pad="98"/>
<connect gate="G$1" pin="P2-0" pad="14"/>
<connect gate="G$1" pin="P2-1" pad="15"/>
<connect gate="G$1" pin="P2-2" pad="16"/>
<connect gate="G$1" pin="P2-3" pad="17"/>
<connect gate="G$1" pin="P2-4" pad="18"/>
<connect gate="G$1" pin="P2-5" pad="19"/>
<connect gate="G$1" pin="P2-6" pad="20"/>
<connect gate="G$1" pin="P2-7" pad="21"/>
<connect gate="G$1" pin="P3-0" pad="90"/>
<connect gate="G$1" pin="P3-1" pad="91"/>
<connect gate="G$1" pin="P3-2" pad="92"/>
<connect gate="G$1" pin="P3-3" pad="93"/>
<connect gate="G$1" pin="P3-4" pad="94"/>
<connect gate="G$1" pin="P3-5" pad="95"/>
<connect gate="G$1" pin="P3-6" pad="96"/>
<connect gate="G$1" pin="P3-7" pad="97"/>
<connect gate="G$1" pin="P4-0" pad="64"/>
<connect gate="G$1" pin="P4-1" pad="65"/>
<connect gate="G$1" pin="P4-2" pad="66"/>
<connect gate="G$1" pin="P4-3" pad="68"/>
<connect gate="G$1" pin="P4-4" pad="69"/>
<connect gate="G$1" pin="P4-5" pad="70"/>
<connect gate="G$1" pin="P4-6" pad="71"/>
<connect gate="G$1" pin="P4-7" pad="72"/>
<connect gate="G$1" pin="P5-0" pad="44"/>
<connect gate="G$1" pin="P5-1" pad="43"/>
<connect gate="G$1" pin="P5-2" pad="42"/>
<connect gate="G$1" pin="P5-3" pad="41"/>
<connect gate="G$1" pin="P5-4" pad="40"/>
<connect gate="G$1" pin="P5-5" pad="39"/>
<connect gate="G$1" pin="P5-6" pad="38"/>
<connect gate="G$1" pin="P5-7" pad="37"/>
<connect gate="G$1" pin="P6-0" pad="46"/>
<connect gate="G$1" pin="P6-1" pad="47"/>
<connect gate="G$1" pin="P6-2" pad="48"/>
<connect gate="G$1" pin="P6-3" pad="49"/>
<connect gate="G$1" pin="P6-4" pad="50"/>
<connect gate="G$1" pin="P6-5" pad="54"/>
<connect gate="G$1" pin="P6-6" pad="55"/>
<connect gate="G$1" pin="P6-7" pad="56"/>
<connect gate="G$1" pin="P7-0" pad="87"/>
<connect gate="G$1" pin="P7-1" pad="86"/>
<connect gate="G$1" pin="P7-2" pad="85"/>
<connect gate="G$1" pin="P7-3" pad="84"/>
<connect gate="G$1" pin="P7-4" pad="83"/>
<connect gate="G$1" pin="P7-5" pad="82"/>
<connect gate="G$1" pin="P7-6" pad="81"/>
<connect gate="G$1" pin="P7-7" pad="80"/>
<connect gate="G$1" pin="P8-0" pad="57"/>
<connect gate="G$1" pin="P8-1" pad="58"/>
<connect gate="G$1" pin="P8-2" pad="59"/>
<connect gate="G$1" pin="P8-3" pad="60"/>
<connect gate="G$1" pin="VAGND" pad="79"/>
<connect gate="G$1" pin="VAREF" pad="78"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
<connect gate="P" pin="VCC@1" pad="11"/>
<connect gate="P" pin="VCC@2" pad="63"/>
<connect gate="P" pin="VSS@1" pad="10"/>
<connect gate="P" pin="VSS@2" pad="62"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C517NA" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C517NA"/>
<gate name="P" symbol="2VCC2VSS"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="G$1" pin="!EA" pad="51"/>
<connect gate="G$1" pin="!HWPD" pad="60"/>
<connect gate="G$1" pin="!PE!/SWD" pad="4"/>
<connect gate="G$1" pin="!PSEN" pad="49"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="!RO" pad="82"/>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="OWE" pad="69"/>
<connect gate="G$1" pin="P0-0" pad="52"/>
<connect gate="G$1" pin="P0-1" pad="53"/>
<connect gate="G$1" pin="P0-2" pad="54"/>
<connect gate="G$1" pin="P0-3" pad="55"/>
<connect gate="G$1" pin="P0-4" pad="56"/>
<connect gate="G$1" pin="P0-5" pad="57"/>
<connect gate="G$1" pin="P0-6" pad="58"/>
<connect gate="G$1" pin="P0-7" pad="59"/>
<connect gate="G$1" pin="P1-0" pad="36"/>
<connect gate="G$1" pin="P1-1" pad="35"/>
<connect gate="G$1" pin="P1-2" pad="34"/>
<connect gate="G$1" pin="P1-3" pad="33"/>
<connect gate="G$1" pin="P1-4" pad="32"/>
<connect gate="G$1" pin="P1-5" pad="31"/>
<connect gate="G$1" pin="P1-6" pad="30"/>
<connect gate="G$1" pin="P1-7" pad="29"/>
<connect gate="G$1" pin="P2-0" pad="41"/>
<connect gate="G$1" pin="P2-1" pad="42"/>
<connect gate="G$1" pin="P2-2" pad="43"/>
<connect gate="G$1" pin="P2-3" pad="44"/>
<connect gate="G$1" pin="P2-4" pad="45"/>
<connect gate="G$1" pin="P2-5" pad="46"/>
<connect gate="G$1" pin="P2-6" pad="47"/>
<connect gate="G$1" pin="P2-7" pad="48"/>
<connect gate="G$1" pin="P3-0" pad="21"/>
<connect gate="G$1" pin="P3-1" pad="22"/>
<connect gate="G$1" pin="P3-2" pad="23"/>
<connect gate="G$1" pin="P3-3" pad="24"/>
<connect gate="G$1" pin="P3-4" pad="25"/>
<connect gate="G$1" pin="P3-5" pad="26"/>
<connect gate="G$1" pin="P3-6" pad="27"/>
<connect gate="G$1" pin="P3-7" pad="28"/>
<connect gate="G$1" pin="P4-0" pad="1"/>
<connect gate="G$1" pin="P4-1" pad="2"/>
<connect gate="G$1" pin="P4-2" pad="3"/>
<connect gate="G$1" pin="P4-3" pad="5"/>
<connect gate="G$1" pin="P4-4" pad="6"/>
<connect gate="G$1" pin="P4-5" pad="7"/>
<connect gate="G$1" pin="P4-6" pad="8"/>
<connect gate="G$1" pin="P4-7" pad="9"/>
<connect gate="G$1" pin="P5-0" pad="68"/>
<connect gate="G$1" pin="P5-1" pad="67"/>
<connect gate="G$1" pin="P5-2" pad="66"/>
<connect gate="G$1" pin="P5-3" pad="65"/>
<connect gate="G$1" pin="P5-4" pad="64"/>
<connect gate="G$1" pin="P5-5" pad="63"/>
<connect gate="G$1" pin="P5-6" pad="62"/>
<connect gate="G$1" pin="P5-7" pad="61"/>
<connect gate="G$1" pin="P6-0" pad="70"/>
<connect gate="G$1" pin="P6-1" pad="71"/>
<connect gate="G$1" pin="P6-2" pad="72"/>
<connect gate="G$1" pin="P6-3" pad="73"/>
<connect gate="G$1" pin="P6-4" pad="74"/>
<connect gate="G$1" pin="P6-5" pad="75"/>
<connect gate="G$1" pin="P6-6" pad="76"/>
<connect gate="G$1" pin="P6-7" pad="77"/>
<connect gate="G$1" pin="P7-0" pad="20"/>
<connect gate="G$1" pin="P7-1" pad="19"/>
<connect gate="G$1" pin="P7-2" pad="18"/>
<connect gate="G$1" pin="P7-3" pad="17"/>
<connect gate="G$1" pin="P7-4" pad="16"/>
<connect gate="G$1" pin="P7-5" pad="15"/>
<connect gate="G$1" pin="P7-6" pad="14"/>
<connect gate="G$1" pin="P7-7" pad="13"/>
<connect gate="G$1" pin="P8-0" pad="78"/>
<connect gate="G$1" pin="P8-1" pad="79"/>
<connect gate="G$1" pin="P8-2" pad="80"/>
<connect gate="G$1" pin="P8-3" pad="81"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="VCC@1" pad="38"/>
<connect gate="P" pin="VCC@2" pad="84"/>
<connect gate="P" pin="VSS@1" pad="37"/>
<connect gate="P" pin="VSS@2" pad="83"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SOC" package="PLCC84SOCK">
<connects>
<connect gate="G$1" pin="!EA" pad="51"/>
<connect gate="G$1" pin="!HWPD" pad="60"/>
<connect gate="G$1" pin="!PE!/SWD" pad="4"/>
<connect gate="G$1" pin="!PSEN" pad="49"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="!RO" pad="82"/>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="OWE" pad="69"/>
<connect gate="G$1" pin="P0-0" pad="52"/>
<connect gate="G$1" pin="P0-1" pad="53"/>
<connect gate="G$1" pin="P0-2" pad="54"/>
<connect gate="G$1" pin="P0-3" pad="55"/>
<connect gate="G$1" pin="P0-4" pad="56"/>
<connect gate="G$1" pin="P0-5" pad="57"/>
<connect gate="G$1" pin="P0-6" pad="58"/>
<connect gate="G$1" pin="P0-7" pad="59"/>
<connect gate="G$1" pin="P1-0" pad="36"/>
<connect gate="G$1" pin="P1-1" pad="35"/>
<connect gate="G$1" pin="P1-2" pad="34"/>
<connect gate="G$1" pin="P1-3" pad="33"/>
<connect gate="G$1" pin="P1-4" pad="32"/>
<connect gate="G$1" pin="P1-5" pad="31"/>
<connect gate="G$1" pin="P1-6" pad="30"/>
<connect gate="G$1" pin="P1-7" pad="29"/>
<connect gate="G$1" pin="P2-0" pad="41"/>
<connect gate="G$1" pin="P2-1" pad="42"/>
<connect gate="G$1" pin="P2-2" pad="43"/>
<connect gate="G$1" pin="P2-3" pad="44"/>
<connect gate="G$1" pin="P2-4" pad="45"/>
<connect gate="G$1" pin="P2-5" pad="46"/>
<connect gate="G$1" pin="P2-6" pad="47"/>
<connect gate="G$1" pin="P2-7" pad="48"/>
<connect gate="G$1" pin="P3-0" pad="21"/>
<connect gate="G$1" pin="P3-1" pad="22"/>
<connect gate="G$1" pin="P3-2" pad="23"/>
<connect gate="G$1" pin="P3-3" pad="24"/>
<connect gate="G$1" pin="P3-4" pad="25"/>
<connect gate="G$1" pin="P3-5" pad="26"/>
<connect gate="G$1" pin="P3-6" pad="27"/>
<connect gate="G$1" pin="P3-7" pad="28"/>
<connect gate="G$1" pin="P4-0" pad="1"/>
<connect gate="G$1" pin="P4-1" pad="2"/>
<connect gate="G$1" pin="P4-2" pad="3"/>
<connect gate="G$1" pin="P4-3" pad="5"/>
<connect gate="G$1" pin="P4-4" pad="6"/>
<connect gate="G$1" pin="P4-5" pad="7"/>
<connect gate="G$1" pin="P4-6" pad="8"/>
<connect gate="G$1" pin="P4-7" pad="9"/>
<connect gate="G$1" pin="P5-0" pad="68"/>
<connect gate="G$1" pin="P5-1" pad="67"/>
<connect gate="G$1" pin="P5-2" pad="66"/>
<connect gate="G$1" pin="P5-3" pad="65"/>
<connect gate="G$1" pin="P5-4" pad="64"/>
<connect gate="G$1" pin="P5-5" pad="63"/>
<connect gate="G$1" pin="P5-6" pad="62"/>
<connect gate="G$1" pin="P5-7" pad="61"/>
<connect gate="G$1" pin="P6-0" pad="70"/>
<connect gate="G$1" pin="P6-1" pad="71"/>
<connect gate="G$1" pin="P6-2" pad="72"/>
<connect gate="G$1" pin="P6-3" pad="73"/>
<connect gate="G$1" pin="P6-4" pad="74"/>
<connect gate="G$1" pin="P6-5" pad="75"/>
<connect gate="G$1" pin="P6-6" pad="76"/>
<connect gate="G$1" pin="P6-7" pad="77"/>
<connect gate="G$1" pin="P7-0" pad="20"/>
<connect gate="G$1" pin="P7-1" pad="19"/>
<connect gate="G$1" pin="P7-2" pad="18"/>
<connect gate="G$1" pin="P7-3" pad="17"/>
<connect gate="G$1" pin="P7-4" pad="16"/>
<connect gate="G$1" pin="P7-5" pad="15"/>
<connect gate="G$1" pin="P7-6" pad="14"/>
<connect gate="G$1" pin="P7-7" pad="13"/>
<connect gate="G$1" pin="P8-0" pad="78"/>
<connect gate="G$1" pin="P8-1" pad="79"/>
<connect gate="G$1" pin="P8-2" pad="80"/>
<connect gate="G$1" pin="P8-3" pad="81"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="VCC@1" pad="38"/>
<connect gate="P" pin="VCC@2" pad="84"/>
<connect gate="P" pin="VSS@1" pad="37"/>
<connect gate="P" pin="VSS@2" pad="83"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C517MA" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C517MA"/>
<gate name="P" symbol="2VCC2VSS"/>
</gates>
<devices>
<device name="" package="MQFP100">
<connects>
<connect gate="G$1" pin="!EA" pad="24"/>
<connect gate="G$1" pin="!HWPD" pad="36"/>
<connect gate="G$1" pin="!PE!/SWD" pad="67"/>
<connect gate="G$1" pin="!PSEN" pad="22"/>
<connect gate="G$1" pin="!RESET" pad="73"/>
<connect gate="G$1" pin="!RO" pad="61"/>
<connect gate="G$1" pin="ALE" pad="23"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@10" pad="53"/>
<connect gate="G$1" pin="NC@11" pad="74"/>
<connect gate="G$1" pin="NC@12" pad="75"/>
<connect gate="G$1" pin="NC@13" pad="76"/>
<connect gate="G$1" pin="NC@14" pad="77"/>
<connect gate="G$1" pin="NC@15" pad="88"/>
<connect gate="G$1" pin="NC@16" pad="89"/>
<connect gate="G$1" pin="NC@2" pad="3"/>
<connect gate="G$1" pin="NC@3" pad="4"/>
<connect gate="G$1" pin="NC@4" pad="5"/>
<connect gate="G$1" pin="NC@5" pad="25"/>
<connect gate="G$1" pin="NC@6" pad="28"/>
<connect gate="G$1" pin="NC@7" pad="29"/>
<connect gate="G$1" pin="NC@8" pad="51"/>
<connect gate="G$1" pin="NC@9" pad="52"/>
<connect gate="G$1" pin="OWE" pad="45"/>
<connect gate="G$1" pin="P0-0" pad="26"/>
<connect gate="G$1" pin="P0-1" pad="27"/>
<connect gate="G$1" pin="P0-2" pad="30"/>
<connect gate="G$1" pin="P0-3" pad="31"/>
<connect gate="G$1" pin="P0-4" pad="32"/>
<connect gate="G$1" pin="P0-5" pad="33"/>
<connect gate="G$1" pin="P0-6" pad="34"/>
<connect gate="G$1" pin="P0-7" pad="35"/>
<connect gate="G$1" pin="P1-0" pad="9"/>
<connect gate="G$1" pin="P1-1" pad="8"/>
<connect gate="G$1" pin="P1-2" pad="7"/>
<connect gate="G$1" pin="P1-3" pad="6"/>
<connect gate="G$1" pin="P1-4" pad="1"/>
<connect gate="G$1" pin="P1-5" pad="100"/>
<connect gate="G$1" pin="P1-6" pad="99"/>
<connect gate="G$1" pin="P1-7" pad="98"/>
<connect gate="G$1" pin="P2-0" pad="14"/>
<connect gate="G$1" pin="P2-1" pad="15"/>
<connect gate="G$1" pin="P2-2" pad="16"/>
<connect gate="G$1" pin="P2-3" pad="17"/>
<connect gate="G$1" pin="P2-4" pad="18"/>
<connect gate="G$1" pin="P2-5" pad="19"/>
<connect gate="G$1" pin="P2-6" pad="20"/>
<connect gate="G$1" pin="P2-7" pad="21"/>
<connect gate="G$1" pin="P3-0" pad="90"/>
<connect gate="G$1" pin="P3-1" pad="91"/>
<connect gate="G$1" pin="P3-2" pad="92"/>
<connect gate="G$1" pin="P3-3" pad="93"/>
<connect gate="G$1" pin="P3-4" pad="94"/>
<connect gate="G$1" pin="P3-5" pad="95"/>
<connect gate="G$1" pin="P3-6" pad="96"/>
<connect gate="G$1" pin="P3-7" pad="97"/>
<connect gate="G$1" pin="P4-0" pad="64"/>
<connect gate="G$1" pin="P4-1" pad="65"/>
<connect gate="G$1" pin="P4-2" pad="66"/>
<connect gate="G$1" pin="P4-3" pad="68"/>
<connect gate="G$1" pin="P4-4" pad="69"/>
<connect gate="G$1" pin="P4-5" pad="70"/>
<connect gate="G$1" pin="P4-6" pad="71"/>
<connect gate="G$1" pin="P4-7" pad="72"/>
<connect gate="G$1" pin="P5-0" pad="44"/>
<connect gate="G$1" pin="P5-1" pad="43"/>
<connect gate="G$1" pin="P5-2" pad="42"/>
<connect gate="G$1" pin="P5-3" pad="41"/>
<connect gate="G$1" pin="P5-4" pad="40"/>
<connect gate="G$1" pin="P5-5" pad="39"/>
<connect gate="G$1" pin="P5-6" pad="38"/>
<connect gate="G$1" pin="P5-7" pad="37"/>
<connect gate="G$1" pin="P6-0" pad="46"/>
<connect gate="G$1" pin="P6-1" pad="47"/>
<connect gate="G$1" pin="P6-2" pad="48"/>
<connect gate="G$1" pin="P6-3" pad="49"/>
<connect gate="G$1" pin="P6-4" pad="50"/>
<connect gate="G$1" pin="P6-5" pad="54"/>
<connect gate="G$1" pin="P6-6" pad="55"/>
<connect gate="G$1" pin="P6-7" pad="56"/>
<connect gate="G$1" pin="P7-0" pad="87"/>
<connect gate="G$1" pin="P7-1" pad="86"/>
<connect gate="G$1" pin="P7-2" pad="85"/>
<connect gate="G$1" pin="P7-3" pad="84"/>
<connect gate="G$1" pin="P7-4" pad="83"/>
<connect gate="G$1" pin="P7-5" pad="82"/>
<connect gate="G$1" pin="P7-6" pad="81"/>
<connect gate="G$1" pin="P7-7" pad="80"/>
<connect gate="G$1" pin="P8-0" pad="57"/>
<connect gate="G$1" pin="P8-1" pad="58"/>
<connect gate="G$1" pin="P8-2" pad="59"/>
<connect gate="G$1" pin="P8-3" pad="60"/>
<connect gate="G$1" pin="VAGND" pad="79"/>
<connect gate="G$1" pin="VAREF" pad="78"/>
<connect gate="G$1" pin="XTAL1" pad="13"/>
<connect gate="G$1" pin="XTAL2" pad="12"/>
<connect gate="P" pin="VCC@1" pad="11"/>
<connect gate="P" pin="VCC@2" pad="63"/>
<connect gate="P" pin="VSS@1" pad="10"/>
<connect gate="P" pin="VSS@2" pad="62"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80515-N" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80515-N"/>
<gate name="P" symbol="VCCVSS"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!EA" pad="60"/>
<connect gate="G$1" pin="!PSEN" pad="58"/>
<connect gate="G$1" pin="!RESET" pad="19"/>
<connect gate="G$1" pin="ALE" pad="59"/>
<connect gate="G$1" pin="AN0" pad="29"/>
<connect gate="G$1" pin="AN1" pad="28"/>
<connect gate="G$1" pin="AN2" pad="27"/>
<connect gate="G$1" pin="AN3" pad="26"/>
<connect gate="G$1" pin="AN4" pad="25"/>
<connect gate="G$1" pin="AN5" pad="24"/>
<connect gate="G$1" pin="AN6" pad="23"/>
<connect gate="G$1" pin="AN7" pad="22"/>
<connect gate="G$1" pin="P0-0" pad="61"/>
<connect gate="G$1" pin="P0-1" pad="62"/>
<connect gate="G$1" pin="P0-2" pad="63"/>
<connect gate="G$1" pin="P0-3" pad="64"/>
<connect gate="G$1" pin="P0-4" pad="65"/>
<connect gate="G$1" pin="P0-5" pad="66"/>
<connect gate="G$1" pin="P0-6" pad="67"/>
<connect gate="G$1" pin="P0-7" pad="68"/>
<connect gate="G$1" pin="P1-0" pad="45"/>
<connect gate="G$1" pin="P1-1" pad="44"/>
<connect gate="G$1" pin="P1-2" pad="43"/>
<connect gate="G$1" pin="P1-3" pad="42"/>
<connect gate="G$1" pin="P1-4" pad="41"/>
<connect gate="G$1" pin="P1-5" pad="40"/>
<connect gate="G$1" pin="P1-6" pad="39"/>
<connect gate="G$1" pin="P1-7" pad="38"/>
<connect gate="G$1" pin="P2-0" pad="50"/>
<connect gate="G$1" pin="P2-1" pad="51"/>
<connect gate="G$1" pin="P2-2" pad="52"/>
<connect gate="G$1" pin="P2-3" pad="53"/>
<connect gate="G$1" pin="P2-4" pad="54"/>
<connect gate="G$1" pin="P2-5" pad="55"/>
<connect gate="G$1" pin="P2-6" pad="56"/>
<connect gate="G$1" pin="P2-7" pad="57"/>
<connect gate="G$1" pin="P3-0" pad="30"/>
<connect gate="G$1" pin="P3-1" pad="31"/>
<connect gate="G$1" pin="P3-2" pad="32"/>
<connect gate="G$1" pin="P3-3" pad="33"/>
<connect gate="G$1" pin="P3-4" pad="34"/>
<connect gate="G$1" pin="P3-5" pad="35"/>
<connect gate="G$1" pin="P3-6" pad="36"/>
<connect gate="G$1" pin="P3-7" pad="37"/>
<connect gate="G$1" pin="P4-0" pad="10"/>
<connect gate="G$1" pin="P4-1" pad="11"/>
<connect gate="G$1" pin="P4-2" pad="12"/>
<connect gate="G$1" pin="P4-3" pad="14"/>
<connect gate="G$1" pin="P4-4" pad="15"/>
<connect gate="G$1" pin="P4-5" pad="16"/>
<connect gate="G$1" pin="P4-6" pad="17"/>
<connect gate="G$1" pin="P4-7" pad="18"/>
<connect gate="G$1" pin="P5-0" pad="8"/>
<connect gate="G$1" pin="P5-1" pad="7"/>
<connect gate="G$1" pin="P5-2" pad="6"/>
<connect gate="G$1" pin="P5-3" pad="5"/>
<connect gate="G$1" pin="P5-4" pad="4"/>
<connect gate="G$1" pin="P5-5" pad="3"/>
<connect gate="G$1" pin="P5-6" pad="2"/>
<connect gate="G$1" pin="P5-7" pad="1"/>
<connect gate="G$1" pin="VAGND" pad="21"/>
<connect gate="G$1" pin="VAREF" pad="20"/>
<connect gate="G$1" pin="VBB" pad="46"/>
<connect gate="G$1" pin="VPD" pad="13"/>
<connect gate="G$1" pin="XTAL1" pad="49"/>
<connect gate="G$1" pin="XTAL2" pad="48"/>
<connect gate="P" pin="VCC" pad="9"/>
<connect gate="P" pin="VSS" pad="47"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C515-A" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C515-A"/>
<gate name="P" symbol="VCCVSS"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!EA" pad="51"/>
<connect gate="G$1" pin="!HWPD" pad="68"/>
<connect gate="G$1" pin="!PE!/SWD" pad="4"/>
<connect gate="G$1" pin="!PSEN" pad="49"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="P0-0" pad="52"/>
<connect gate="G$1" pin="P0-1" pad="53"/>
<connect gate="G$1" pin="P0-2" pad="54"/>
<connect gate="G$1" pin="P0-3" pad="55"/>
<connect gate="G$1" pin="P0-4" pad="56"/>
<connect gate="G$1" pin="P0-5" pad="57"/>
<connect gate="G$1" pin="P0-6" pad="58"/>
<connect gate="G$1" pin="P0-7" pad="59"/>
<connect gate="G$1" pin="P1-0" pad="36"/>
<connect gate="G$1" pin="P1-1" pad="35"/>
<connect gate="G$1" pin="P1-2" pad="34"/>
<connect gate="G$1" pin="P1-3" pad="33"/>
<connect gate="G$1" pin="P1-4" pad="32"/>
<connect gate="G$1" pin="P1-5" pad="31"/>
<connect gate="G$1" pin="P1-6" pad="30"/>
<connect gate="G$1" pin="P1-7" pad="29"/>
<connect gate="G$1" pin="P2-0" pad="41"/>
<connect gate="G$1" pin="P2-1" pad="42"/>
<connect gate="G$1" pin="P2-2" pad="43"/>
<connect gate="G$1" pin="P2-3" pad="44"/>
<connect gate="G$1" pin="P2-4" pad="45"/>
<connect gate="G$1" pin="P2-5" pad="46"/>
<connect gate="G$1" pin="P2-6" pad="47"/>
<connect gate="G$1" pin="P2-7" pad="48"/>
<connect gate="G$1" pin="P3-0" pad="21"/>
<connect gate="G$1" pin="P3-1" pad="22"/>
<connect gate="G$1" pin="P3-2" pad="23"/>
<connect gate="G$1" pin="P3-3" pad="24"/>
<connect gate="G$1" pin="P3-4" pad="25"/>
<connect gate="G$1" pin="P3-5" pad="26"/>
<connect gate="G$1" pin="P3-6" pad="27"/>
<connect gate="G$1" pin="P3-7" pad="28"/>
<connect gate="G$1" pin="P4-0" pad="1"/>
<connect gate="G$1" pin="P4-1" pad="2"/>
<connect gate="G$1" pin="P4-2" pad="3"/>
<connect gate="G$1" pin="P4-3" pad="5"/>
<connect gate="G$1" pin="P4-4" pad="6"/>
<connect gate="G$1" pin="P4-5" pad="7"/>
<connect gate="G$1" pin="P4-6" pad="8"/>
<connect gate="G$1" pin="P4-7" pad="9"/>
<connect gate="G$1" pin="P5-0" pad="67"/>
<connect gate="G$1" pin="P5-1" pad="66"/>
<connect gate="G$1" pin="P5-2" pad="65"/>
<connect gate="G$1" pin="P5-3" pad="64"/>
<connect gate="G$1" pin="P5-4" pad="63"/>
<connect gate="G$1" pin="P5-5" pad="62"/>
<connect gate="G$1" pin="P5-6" pad="61"/>
<connect gate="G$1" pin="P5-7" pad="60"/>
<connect gate="G$1" pin="P6-0" pad="20"/>
<connect gate="G$1" pin="P6-1" pad="19"/>
<connect gate="G$1" pin="P6-2" pad="18"/>
<connect gate="G$1" pin="P6-3" pad="17"/>
<connect gate="G$1" pin="P6-4" pad="16"/>
<connect gate="G$1" pin="P6-5" pad="15"/>
<connect gate="G$1" pin="P6-6" pad="14"/>
<connect gate="G$1" pin="P6-7" pad="13"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="VCC" pad="37"/>
<connect gate="P" pin="VSS" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SOCK" package="PLCC68SOCK">
<connects>
<connect gate="G$1" pin="!EA" pad="51"/>
<connect gate="G$1" pin="!HWPD" pad="68"/>
<connect gate="G$1" pin="!PE!/SWD" pad="4"/>
<connect gate="G$1" pin="!PSEN" pad="49"/>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="P0-0" pad="52"/>
<connect gate="G$1" pin="P0-1" pad="53"/>
<connect gate="G$1" pin="P0-2" pad="54"/>
<connect gate="G$1" pin="P0-3" pad="55"/>
<connect gate="G$1" pin="P0-4" pad="56"/>
<connect gate="G$1" pin="P0-5" pad="57"/>
<connect gate="G$1" pin="P0-6" pad="58"/>
<connect gate="G$1" pin="P0-7" pad="59"/>
<connect gate="G$1" pin="P1-0" pad="36"/>
<connect gate="G$1" pin="P1-1" pad="35"/>
<connect gate="G$1" pin="P1-2" pad="34"/>
<connect gate="G$1" pin="P1-3" pad="33"/>
<connect gate="G$1" pin="P1-4" pad="32"/>
<connect gate="G$1" pin="P1-5" pad="31"/>
<connect gate="G$1" pin="P1-6" pad="30"/>
<connect gate="G$1" pin="P1-7" pad="29"/>
<connect gate="G$1" pin="P2-0" pad="41"/>
<connect gate="G$1" pin="P2-1" pad="42"/>
<connect gate="G$1" pin="P2-2" pad="43"/>
<connect gate="G$1" pin="P2-3" pad="44"/>
<connect gate="G$1" pin="P2-4" pad="45"/>
<connect gate="G$1" pin="P2-5" pad="46"/>
<connect gate="G$1" pin="P2-6" pad="47"/>
<connect gate="G$1" pin="P2-7" pad="48"/>
<connect gate="G$1" pin="P3-0" pad="21"/>
<connect gate="G$1" pin="P3-1" pad="22"/>
<connect gate="G$1" pin="P3-2" pad="23"/>
<connect gate="G$1" pin="P3-3" pad="24"/>
<connect gate="G$1" pin="P3-4" pad="25"/>
<connect gate="G$1" pin="P3-5" pad="26"/>
<connect gate="G$1" pin="P3-6" pad="27"/>
<connect gate="G$1" pin="P3-7" pad="28"/>
<connect gate="G$1" pin="P4-0" pad="1"/>
<connect gate="G$1" pin="P4-1" pad="2"/>
<connect gate="G$1" pin="P4-2" pad="3"/>
<connect gate="G$1" pin="P4-3" pad="5"/>
<connect gate="G$1" pin="P4-4" pad="6"/>
<connect gate="G$1" pin="P4-5" pad="7"/>
<connect gate="G$1" pin="P4-6" pad="8"/>
<connect gate="G$1" pin="P4-7" pad="9"/>
<connect gate="G$1" pin="P5-0" pad="67"/>
<connect gate="G$1" pin="P5-1" pad="66"/>
<connect gate="G$1" pin="P5-2" pad="65"/>
<connect gate="G$1" pin="P5-3" pad="64"/>
<connect gate="G$1" pin="P5-4" pad="63"/>
<connect gate="G$1" pin="P5-5" pad="62"/>
<connect gate="G$1" pin="P5-6" pad="61"/>
<connect gate="G$1" pin="P5-7" pad="60"/>
<connect gate="G$1" pin="P6-0" pad="20"/>
<connect gate="G$1" pin="P6-1" pad="19"/>
<connect gate="G$1" pin="P6-2" pad="18"/>
<connect gate="G$1" pin="P6-3" pad="17"/>
<connect gate="G$1" pin="P6-4" pad="16"/>
<connect gate="G$1" pin="P6-5" pad="15"/>
<connect gate="G$1" pin="P6-6" pad="14"/>
<connect gate="G$1" pin="P6-7" pad="13"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="VCC" pad="37"/>
<connect gate="P" pin="VSS" pad="38"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C501-LN" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C501-LN"/>
<gate name="P" symbol="VCCVSS"/>
</gates>
<devices>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="!EA" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="32"/>
<connect gate="G$1" pin="ALE" pad="33"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@2" pad="12"/>
<connect gate="G$1" pin="NC@3" pad="23"/>
<connect gate="G$1" pin="NC@4" pad="34"/>
<connect gate="G$1" pin="P0-0" pad="43"/>
<connect gate="G$1" pin="P0-1" pad="42"/>
<connect gate="G$1" pin="P0-2" pad="41"/>
<connect gate="G$1" pin="P0-3" pad="40"/>
<connect gate="G$1" pin="P0-4" pad="39"/>
<connect gate="G$1" pin="P0-5" pad="38"/>
<connect gate="G$1" pin="P0-6" pad="37"/>
<connect gate="G$1" pin="P0-7" pad="36"/>
<connect gate="G$1" pin="P1-0" pad="2"/>
<connect gate="G$1" pin="P1-1" pad="3"/>
<connect gate="G$1" pin="P1-2" pad="4"/>
<connect gate="G$1" pin="P1-3" pad="5"/>
<connect gate="G$1" pin="P1-4" pad="6"/>
<connect gate="G$1" pin="P1-5" pad="7"/>
<connect gate="G$1" pin="P1-6" pad="8"/>
<connect gate="G$1" pin="P1-7" pad="9"/>
<connect gate="G$1" pin="P2-0" pad="24"/>
<connect gate="G$1" pin="P2-1" pad="25"/>
<connect gate="G$1" pin="P2-2" pad="26"/>
<connect gate="G$1" pin="P2-3" pad="27"/>
<connect gate="G$1" pin="P2-4" pad="28"/>
<connect gate="G$1" pin="P2-5" pad="29"/>
<connect gate="G$1" pin="P2-6" pad="30"/>
<connect gate="G$1" pin="P2-7" pad="31"/>
<connect gate="G$1" pin="P3-0" pad="11"/>
<connect gate="G$1" pin="P3-1" pad="13"/>
<connect gate="G$1" pin="P3-2" pad="14"/>
<connect gate="G$1" pin="P3-3" pad="15"/>
<connect gate="G$1" pin="P3-4" pad="16"/>
<connect gate="G$1" pin="P3-5" pad="17"/>
<connect gate="G$1" pin="P3-6" pad="18"/>
<connect gate="G$1" pin="P3-7" pad="19"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="XTAL1" pad="21"/>
<connect gate="G$1" pin="XTAL2" pad="20"/>
<connect gate="P" pin="VCC" pad="44"/>
<connect gate="P" pin="VSS" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C501-LP" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C501-LP"/>
<gate name="P" symbol="VCCVSS"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!EA" pad="31"/>
<connect gate="G$1" pin="!PSEN" pad="29"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="P0-0" pad="39"/>
<connect gate="G$1" pin="P0-1" pad="38"/>
<connect gate="G$1" pin="P0-2" pad="37"/>
<connect gate="G$1" pin="P0-3" pad="36"/>
<connect gate="G$1" pin="P0-4" pad="35"/>
<connect gate="G$1" pin="P0-5" pad="34"/>
<connect gate="G$1" pin="P0-6" pad="33"/>
<connect gate="G$1" pin="P0-7" pad="32"/>
<connect gate="G$1" pin="P1-0" pad="1"/>
<connect gate="G$1" pin="P1-1" pad="2"/>
<connect gate="G$1" pin="P1-2" pad="3"/>
<connect gate="G$1" pin="P1-3" pad="4"/>
<connect gate="G$1" pin="P1-4" pad="5"/>
<connect gate="G$1" pin="P1-5" pad="6"/>
<connect gate="G$1" pin="P1-6" pad="7"/>
<connect gate="G$1" pin="P1-7" pad="8"/>
<connect gate="G$1" pin="P2-0" pad="21"/>
<connect gate="G$1" pin="P2-1" pad="22"/>
<connect gate="G$1" pin="P2-2" pad="23"/>
<connect gate="G$1" pin="P2-3" pad="24"/>
<connect gate="G$1" pin="P2-4" pad="25"/>
<connect gate="G$1" pin="P2-5" pad="26"/>
<connect gate="G$1" pin="P2-6" pad="27"/>
<connect gate="G$1" pin="P2-7" pad="28"/>
<connect gate="G$1" pin="P3-0" pad="10"/>
<connect gate="G$1" pin="P3-1" pad="11"/>
<connect gate="G$1" pin="P3-2" pad="12"/>
<connect gate="G$1" pin="P3-3" pad="13"/>
<connect gate="G$1" pin="P3-4" pad="14"/>
<connect gate="G$1" pin="P3-5" pad="15"/>
<connect gate="G$1" pin="P3-6" pad="16"/>
<connect gate="G$1" pin="P3-7" pad="17"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="XTAL1" pad="19"/>
<connect gate="G$1" pin="XTAL2" pad="18"/>
<connect gate="P" pin="VCC" pad="40"/>
<connect gate="P" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="C503-LN" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C503-LN"/>
<gate name="P" symbol="1VCC2VSS"/>
</gates>
<devices>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="!EA" pad="35"/>
<connect gate="G$1" pin="!PSEN" pad="33"/>
<connect gate="G$1" pin="ALE" pad="34"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="P0-0" pad="43"/>
<connect gate="G$1" pin="P0-1" pad="42"/>
<connect gate="G$1" pin="P0-2" pad="41"/>
<connect gate="G$1" pin="P0-3" pad="40"/>
<connect gate="G$1" pin="P0-4" pad="39"/>
<connect gate="G$1" pin="P0-5" pad="38"/>
<connect gate="G$1" pin="P0-6" pad="37"/>
<connect gate="G$1" pin="P0-7" pad="36"/>
<connect gate="G$1" pin="P1-0" pad="5"/>
<connect gate="G$1" pin="P1-1" pad="6"/>
<connect gate="G$1" pin="P1-2" pad="7"/>
<connect gate="G$1" pin="P1-3" pad="8"/>
<connect gate="G$1" pin="P1-4" pad="9"/>
<connect gate="G$1" pin="P1-5" pad="10"/>
<connect gate="G$1" pin="P1-6" pad="11"/>
<connect gate="G$1" pin="P1-7" pad="12"/>
<connect gate="G$1" pin="P2-0" pad="25"/>
<connect gate="G$1" pin="P2-1" pad="26"/>
<connect gate="G$1" pin="P2-2" pad="27"/>
<connect gate="G$1" pin="P2-3" pad="28"/>
<connect gate="G$1" pin="P2-4" pad="29"/>
<connect gate="G$1" pin="P2-5" pad="30"/>
<connect gate="G$1" pin="P2-6" pad="31"/>
<connect gate="G$1" pin="P2-7" pad="32"/>
<connect gate="G$1" pin="P3-0" pad="14"/>
<connect gate="G$1" pin="P3-1" pad="15"/>
<connect gate="G$1" pin="P3-2" pad="16"/>
<connect gate="G$1" pin="P3-3" pad="17"/>
<connect gate="G$1" pin="P3-4" pad="18"/>
<connect gate="G$1" pin="P3-5" pad="19"/>
<connect gate="G$1" pin="P3-6" pad="20"/>
<connect gate="G$1" pin="P3-7" pad="21"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="G$1" pin="VAGND" pad="3"/>
<connect gate="G$1" pin="VAREF" pad="2"/>
<connect gate="G$1" pin="XTAL1" pad="23"/>
<connect gate="G$1" pin="XTAL2" pad="22"/>
<connect gate="P" pin="VCC" pad="44"/>
<connect gate="P" pin="VSS" pad="24"/>
<connect gate="P" pin="VSS@1" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8085AH" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8085AH"/>
<gate name="P" symbol="VCCVSS"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!INTA" pad="11"/>
<connect gate="G$1" pin="!RD" pad="32"/>
<connect gate="G$1" pin="!RESETIN" pad="36"/>
<connect gate="G$1" pin="!WR" pad="31"/>
<connect gate="G$1" pin="A10" pad="23"/>
<connect gate="G$1" pin="A11" pad="24"/>
<connect gate="G$1" pin="A12" pad="25"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="28"/>
<connect gate="G$1" pin="A8" pad="21"/>
<connect gate="G$1" pin="A9" pad="22"/>
<connect gate="G$1" pin="AD0" pad="12"/>
<connect gate="G$1" pin="AD1" pad="13"/>
<connect gate="G$1" pin="AD2" pad="14"/>
<connect gate="G$1" pin="AD3" pad="15"/>
<connect gate="G$1" pin="AD4" pad="16"/>
<connect gate="G$1" pin="AD5" pad="17"/>
<connect gate="G$1" pin="AD6" pad="18"/>
<connect gate="G$1" pin="AD7" pad="19"/>
<connect gate="G$1" pin="ALE" pad="30"/>
<connect gate="G$1" pin="CLK" pad="37"/>
<connect gate="G$1" pin="HLDA" pad="38"/>
<connect gate="G$1" pin="HOLD" pad="39"/>
<connect gate="G$1" pin="INTR" pad="10"/>
<connect gate="G$1" pin="IO/!M" pad="34"/>
<connect gate="G$1" pin="READY" pad="35"/>
<connect gate="G$1" pin="RESETOUT" pad="3"/>
<connect gate="G$1" pin="RST5-5" pad="9"/>
<connect gate="G$1" pin="RST6-5" pad="8"/>
<connect gate="G$1" pin="RST7-5" pad="7"/>
<connect gate="G$1" pin="S0" pad="29"/>
<connect gate="G$1" pin="S1" pad="33"/>
<connect gate="G$1" pin="SID" pad="5"/>
<connect gate="G$1" pin="SOD" pad="4"/>
<connect gate="G$1" pin="TRAP" pad="6"/>
<connect gate="G$1" pin="X1" pad="1"/>
<connect gate="G$1" pin="X2" pad="2"/>
<connect gate="P" pin="VCC" pad="40"/>
<connect gate="P" pin="VSS" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8088" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8088"/>
<gate name="P" symbol="1VCC2GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!DEN" pad="26"/>
<connect gate="G$1" pin="!INTA" pad="24"/>
<connect gate="G$1" pin="!RD" pad="32"/>
<connect gate="G$1" pin="!SS0" pad="34"/>
<connect gate="G$1" pin="!TEST" pad="23"/>
<connect gate="G$1" pin="!WR" pad="29"/>
<connect gate="G$1" pin="A10" pad="6"/>
<connect gate="G$1" pin="A11" pad="5"/>
<connect gate="G$1" pin="A12" pad="4"/>
<connect gate="G$1" pin="A13" pad="3"/>
<connect gate="G$1" pin="A14" pad="2"/>
<connect gate="G$1" pin="A15" pad="39"/>
<connect gate="G$1" pin="A16" pad="38"/>
<connect gate="G$1" pin="A17" pad="37"/>
<connect gate="G$1" pin="A18" pad="36"/>
<connect gate="G$1" pin="A19" pad="35"/>
<connect gate="G$1" pin="A8" pad="8"/>
<connect gate="G$1" pin="A9" pad="7"/>
<connect gate="G$1" pin="AD0" pad="16"/>
<connect gate="G$1" pin="AD1" pad="15"/>
<connect gate="G$1" pin="AD2" pad="14"/>
<connect gate="G$1" pin="AD3" pad="13"/>
<connect gate="G$1" pin="AD4" pad="12"/>
<connect gate="G$1" pin="AD5" pad="11"/>
<connect gate="G$1" pin="AD6" pad="10"/>
<connect gate="G$1" pin="AD7" pad="9"/>
<connect gate="G$1" pin="ALE" pad="25"/>
<connect gate="G$1" pin="CLK" pad="19"/>
<connect gate="G$1" pin="DT/!R" pad="27"/>
<connect gate="G$1" pin="HLDA" pad="30"/>
<connect gate="G$1" pin="HOLD" pad="31"/>
<connect gate="G$1" pin="INTR" pad="18"/>
<connect gate="G$1" pin="IO/!M" pad="28"/>
<connect gate="G$1" pin="MN/!MX" pad="33"/>
<connect gate="G$1" pin="NMI" pad="17"/>
<connect gate="G$1" pin="READY" pad="22"/>
<connect gate="G$1" pin="RESET" pad="21"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="GND@1" pad="1"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8088-N" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8088-N"/>
<gate name="P" symbol="1VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC44">
<connects>
<connect gate="G$1" pin="!DEN" pad="29"/>
<connect gate="G$1" pin="!INTA" pad="27"/>
<connect gate="G$1" pin="!RD" pad="36"/>
<connect gate="G$1" pin="!SS0" pad="38"/>
<connect gate="G$1" pin="!TEST" pad="26"/>
<connect gate="G$1" pin="!WR" pad="33"/>
<connect gate="G$1" pin="A10" pad="7"/>
<connect gate="G$1" pin="A11" pad="6"/>
<connect gate="G$1" pin="A12" pad="5"/>
<connect gate="G$1" pin="A13" pad="4"/>
<connect gate="G$1" pin="A14" pad="3"/>
<connect gate="G$1" pin="A15" pad="43"/>
<connect gate="G$1" pin="A16" pad="42"/>
<connect gate="G$1" pin="A17" pad="41"/>
<connect gate="G$1" pin="A18" pad="40"/>
<connect gate="G$1" pin="A19" pad="39"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="8"/>
<connect gate="G$1" pin="AD0" pad="17"/>
<connect gate="G$1" pin="AD1" pad="16"/>
<connect gate="G$1" pin="AD2" pad="15"/>
<connect gate="G$1" pin="AD3" pad="14"/>
<connect gate="G$1" pin="AD4" pad="13"/>
<connect gate="G$1" pin="AD5" pad="12"/>
<connect gate="G$1" pin="AD6" pad="11"/>
<connect gate="G$1" pin="AD7" pad="10"/>
<connect gate="G$1" pin="ALE" pad="28"/>
<connect gate="G$1" pin="CLK" pad="21"/>
<connect gate="G$1" pin="DT/!R" pad="31"/>
<connect gate="G$1" pin="HLDA" pad="34"/>
<connect gate="G$1" pin="HOLD" pad="35"/>
<connect gate="G$1" pin="INTR" pad="20"/>
<connect gate="G$1" pin="IO/!M" pad="32"/>
<connect gate="G$1" pin="MN/!MX" pad="37"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@2" pad="18"/>
<connect gate="G$1" pin="NC@3" pad="23"/>
<connect gate="G$1" pin="NC@4" pad="30"/>
<connect gate="G$1" pin="NMI" pad="19"/>
<connect gate="G$1" pin="READY" pad="25"/>
<connect gate="G$1" pin="RESET" pad="24"/>
<connect gate="P" pin="GND" pad="22"/>
<connect gate="P" pin="GND@1" pad="2"/>
<connect gate="P" pin="VCC" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80188" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80188"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!DEN" pad="48"/>
<connect gate="G$1" pin="!LCS" pad="42"/>
<connect gate="G$1" pin="!LOCK" pad="57"/>
<connect gate="G$1" pin="!MCS0" pad="47"/>
<connect gate="G$1" pin="!MCS1" pad="46"/>
<connect gate="G$1" pin="!MCS2" pad="45"/>
<connect gate="G$1" pin="!MCS3" pad="44"/>
<connect gate="G$1" pin="!PCS0" pad="34"/>
<connect gate="G$1" pin="!PCS1" pad="36"/>
<connect gate="G$1" pin="!PCS2" pad="37"/>
<connect gate="G$1" pin="!PCS3" pad="38"/>
<connect gate="G$1" pin="!PCS4" pad="39"/>
<connect gate="G$1" pin="!PCS5!/A1" pad="40"/>
<connect gate="G$1" pin="!PCS6!/A2" pad="41"/>
<connect gate="G$1" pin="!RD!/!QSMD" pad="3"/>
<connect gate="G$1" pin="!RES" pad="33"/>
<connect gate="G$1" pin="!S0" pad="61"/>
<connect gate="G$1" pin="!S1" pad="62"/>
<connect gate="G$1" pin="!S2" pad="63"/>
<connect gate="G$1" pin="!TEST" pad="56"/>
<connect gate="G$1" pin="!UCS" pad="43"/>
<connect gate="G$1" pin="!WR!/QS1" pad="4"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="19"/>
<connect gate="G$1" pin="A12" pad="16"/>
<connect gate="G$1" pin="A13" pad="14"/>
<connect gate="G$1" pin="A14" pad="12"/>
<connect gate="G$1" pin="A15" pad="10"/>
<connect gate="G$1" pin="A16/S3" pad="9"/>
<connect gate="G$1" pin="A17/S4" pad="8"/>
<connect gate="G$1" pin="A18/S5" pad="7"/>
<connect gate="G$1" pin="A19/S6" pad="6"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="23"/>
<connect gate="G$1" pin="AD0" pad="26"/>
<connect gate="G$1" pin="AD1" pad="24"/>
<connect gate="G$1" pin="AD2" pad="22"/>
<connect gate="G$1" pin="AD3" pad="20"/>
<connect gate="G$1" pin="AD4" pad="17"/>
<connect gate="G$1" pin="AD5" pad="15"/>
<connect gate="G$1" pin="AD6" pad="13"/>
<connect gate="G$1" pin="AD7" pad="11"/>
<connect gate="G$1" pin="ALE/QS0" pad="2"/>
<connect gate="G$1" pin="ARDY" pad="64"/>
<connect gate="G$1" pin="CLKOUT" pad="65"/>
<connect gate="G$1" pin="DRQ0" pad="27"/>
<connect gate="G$1" pin="DRQ1" pad="28"/>
<connect gate="G$1" pin="DT/!R" pad="49"/>
<connect gate="G$1" pin="HLDA" pad="60"/>
<connect gate="G$1" pin="HOLD" pad="59"/>
<connect gate="G$1" pin="INT0" pad="54"/>
<connect gate="G$1" pin="INT1" pad="53"/>
<connect gate="G$1" pin="INT2" pad="51"/>
<connect gate="G$1" pin="INT3" pad="50"/>
<connect gate="G$1" pin="NMI" pad="55"/>
<connect gate="G$1" pin="RESET" pad="66"/>
<connect gate="G$1" pin="S7" pad="5"/>
<connect gate="G$1" pin="SRDY" pad="58"/>
<connect gate="G$1" pin="TMRIN0" pad="29"/>
<connect gate="G$1" pin="TMRIN1" pad="30"/>
<connect gate="G$1" pin="TMROUT0" pad="31"/>
<connect gate="G$1" pin="TMROUT1" pad="32"/>
<connect gate="G$1" pin="X1" pad="68"/>
<connect gate="G$1" pin="X2" pad="67"/>
<connect gate="P" pin="GND@1" pad="35"/>
<connect gate="P" pin="GND@2" pad="1"/>
<connect gate="P" pin="VCC@1" pad="18"/>
<connect gate="P" pin="VCC@2" pad="52"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8086" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8086"/>
<gate name="P" symbol="1VCC2GND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!BHE!/S7" pad="34"/>
<connect gate="G$1" pin="!LOCK" pad="29"/>
<connect gate="G$1" pin="!RD" pad="32"/>
<connect gate="G$1" pin="!RQ!/!GT0" pad="31"/>
<connect gate="G$1" pin="!RQ!/!GT1" pad="30"/>
<connect gate="G$1" pin="!S0" pad="26"/>
<connect gate="G$1" pin="!S1" pad="27"/>
<connect gate="G$1" pin="!S2" pad="28"/>
<connect gate="G$1" pin="!TEST" pad="23"/>
<connect gate="G$1" pin="A16/S3" pad="38"/>
<connect gate="G$1" pin="A17/S4" pad="37"/>
<connect gate="G$1" pin="A18/S5" pad="36"/>
<connect gate="G$1" pin="A19/S6" pad="35"/>
<connect gate="G$1" pin="AD0" pad="16"/>
<connect gate="G$1" pin="AD1" pad="15"/>
<connect gate="G$1" pin="AD10" pad="6"/>
<connect gate="G$1" pin="AD11" pad="5"/>
<connect gate="G$1" pin="AD12" pad="4"/>
<connect gate="G$1" pin="AD13" pad="3"/>
<connect gate="G$1" pin="AD14" pad="2"/>
<connect gate="G$1" pin="AD15" pad="39"/>
<connect gate="G$1" pin="AD2" pad="14"/>
<connect gate="G$1" pin="AD3" pad="13"/>
<connect gate="G$1" pin="AD4" pad="12"/>
<connect gate="G$1" pin="AD5" pad="11"/>
<connect gate="G$1" pin="AD6" pad="10"/>
<connect gate="G$1" pin="AD7" pad="9"/>
<connect gate="G$1" pin="AD8" pad="8"/>
<connect gate="G$1" pin="AD9" pad="7"/>
<connect gate="G$1" pin="CLK" pad="19"/>
<connect gate="G$1" pin="INTR" pad="18"/>
<connect gate="G$1" pin="MN/!MX" pad="33"/>
<connect gate="G$1" pin="NMI" pad="17"/>
<connect gate="G$1" pin="QS0" pad="25"/>
<connect gate="G$1" pin="QS1" pad="24"/>
<connect gate="G$1" pin="READY" pad="22"/>
<connect gate="G$1" pin="RESET" pad="21"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="GND@1" pad="1"/>
<connect gate="P" pin="VCC" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80286-N" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80286"/>
<gate name="P" symbol="2VCC3GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!BHE" pad="10"/>
<connect gate="G$1" pin="!BUSY" pad="63"/>
<connect gate="G$1" pin="!ERROR" pad="62"/>
<connect gate="G$1" pin="!LOCK" pad="9"/>
<connect gate="G$1" pin="!PEACK" pad="15"/>
<connect gate="G$1" pin="!READY" pad="4"/>
<connect gate="G$1" pin="!S0" pad="14"/>
<connect gate="G$1" pin="!S1" pad="13"/>
<connect gate="G$1" pin="A0" pad="43"/>
<connect gate="G$1" pin="A1" pad="42"/>
<connect gate="G$1" pin="A10" pad="30"/>
<connect gate="G$1" pin="A11" pad="29"/>
<connect gate="G$1" pin="A12" pad="28"/>
<connect gate="G$1" pin="A13" pad="27"/>
<connect gate="G$1" pin="A14" pad="26"/>
<connect gate="G$1" pin="A15" pad="25"/>
<connect gate="G$1" pin="A16" pad="24"/>
<connect gate="G$1" pin="A17" pad="23"/>
<connect gate="G$1" pin="A18" pad="22"/>
<connect gate="G$1" pin="A19" pad="21"/>
<connect gate="G$1" pin="A2" pad="41"/>
<connect gate="G$1" pin="A20" pad="20"/>
<connect gate="G$1" pin="A21" pad="19"/>
<connect gate="G$1" pin="A22" pad="17"/>
<connect gate="G$1" pin="A23" pad="16"/>
<connect gate="G$1" pin="A3" pad="37"/>
<connect gate="G$1" pin="A4" pad="36"/>
<connect gate="G$1" pin="A5" pad="35"/>
<connect gate="G$1" pin="A6" pad="34"/>
<connect gate="G$1" pin="A7" pad="33"/>
<connect gate="G$1" pin="A8" pad="32"/>
<connect gate="G$1" pin="A9" pad="31"/>
<connect gate="G$1" pin="CAP" pad="61"/>
<connect gate="G$1" pin="CLK" pad="40"/>
<connect gate="G$1" pin="COD/!INTA" pad="7"/>
<connect gate="G$1" pin="D0" pad="45"/>
<connect gate="G$1" pin="D1" pad="47"/>
<connect gate="G$1" pin="D10" pad="50"/>
<connect gate="G$1" pin="D11" pad="52"/>
<connect gate="G$1" pin="D12" pad="54"/>
<connect gate="G$1" pin="D13" pad="56"/>
<connect gate="G$1" pin="D14" pad="58"/>
<connect gate="G$1" pin="D15" pad="60"/>
<connect gate="G$1" pin="D2" pad="49"/>
<connect gate="G$1" pin="D3" pad="51"/>
<connect gate="G$1" pin="D4" pad="53"/>
<connect gate="G$1" pin="D5" pad="55"/>
<connect gate="G$1" pin="D6" pad="57"/>
<connect gate="G$1" pin="D7" pad="59"/>
<connect gate="G$1" pin="D8" pad="46"/>
<connect gate="G$1" pin="D9" pad="48"/>
<connect gate="G$1" pin="HLDA" pad="6"/>
<connect gate="G$1" pin="HOLD" pad="5"/>
<connect gate="G$1" pin="INTR" pad="66"/>
<connect gate="G$1" pin="M/!IO" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="11"/>
<connect gate="G$1" pin="NC@2" pad="12"/>
<connect gate="G$1" pin="NC@3" pad="64"/>
<connect gate="G$1" pin="NC@4" pad="65"/>
<connect gate="G$1" pin="NC@5" pad="67"/>
<connect gate="G$1" pin="NMI" pad="68"/>
<connect gate="G$1" pin="PEREQ" pad="2"/>
<connect gate="G$1" pin="RESET" pad="38"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="44"/>
<connect gate="P" pin="GND@3" pad="1"/>
<connect gate="P" pin="VCC@1" pad="39"/>
<connect gate="P" pin="VCC@2" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80286-A" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80286"/>
<gate name="P" symbol="2VCC3GND"/>
</gates>
<devices>
<device name="" package="PGA68">
<connects>
<connect gate="G$1" pin="!BHE" pad="1"/>
<connect gate="G$1" pin="!BUSY" pad="54"/>
<connect gate="G$1" pin="!ERROR" pad="53"/>
<connect gate="G$1" pin="!LOCK" pad="68"/>
<connect gate="G$1" pin="!PEACK" pad="6"/>
<connect gate="G$1" pin="!READY" pad="63"/>
<connect gate="G$1" pin="!S0" pad="5"/>
<connect gate="G$1" pin="!S1" pad="4"/>
<connect gate="G$1" pin="A0" pad="34"/>
<connect gate="G$1" pin="A1" pad="33"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="20"/>
<connect gate="G$1" pin="A12" pad="19"/>
<connect gate="G$1" pin="A13" pad="18"/>
<connect gate="G$1" pin="A14" pad="17"/>
<connect gate="G$1" pin="A15" pad="16"/>
<connect gate="G$1" pin="A16" pad="15"/>
<connect gate="G$1" pin="A17" pad="14"/>
<connect gate="G$1" pin="A18" pad="13"/>
<connect gate="G$1" pin="A19" pad="12"/>
<connect gate="G$1" pin="A2" pad="32"/>
<connect gate="G$1" pin="A20" pad="11"/>
<connect gate="G$1" pin="A21" pad="10"/>
<connect gate="G$1" pin="A22" pad="8"/>
<connect gate="G$1" pin="A23" pad="7"/>
<connect gate="G$1" pin="A3" pad="28"/>
<connect gate="G$1" pin="A4" pad="27"/>
<connect gate="G$1" pin="A5" pad="26"/>
<connect gate="G$1" pin="A6" pad="25"/>
<connect gate="G$1" pin="A7" pad="24"/>
<connect gate="G$1" pin="A8" pad="23"/>
<connect gate="G$1" pin="A9" pad="22"/>
<connect gate="G$1" pin="CAP" pad="52"/>
<connect gate="G$1" pin="CLK" pad="31"/>
<connect gate="G$1" pin="COD/!INTA" pad="66"/>
<connect gate="G$1" pin="D0" pad="36"/>
<connect gate="G$1" pin="D1" pad="38"/>
<connect gate="G$1" pin="D10" pad="41"/>
<connect gate="G$1" pin="D11" pad="43"/>
<connect gate="G$1" pin="D12" pad="45"/>
<connect gate="G$1" pin="D13" pad="47"/>
<connect gate="G$1" pin="D14" pad="49"/>
<connect gate="G$1" pin="D15" pad="51"/>
<connect gate="G$1" pin="D2" pad="40"/>
<connect gate="G$1" pin="D3" pad="42"/>
<connect gate="G$1" pin="D4" pad="44"/>
<connect gate="G$1" pin="D5" pad="46"/>
<connect gate="G$1" pin="D6" pad="48"/>
<connect gate="G$1" pin="D7" pad="50"/>
<connect gate="G$1" pin="D8" pad="37"/>
<connect gate="G$1" pin="D9" pad="39"/>
<connect gate="G$1" pin="HLDA" pad="65"/>
<connect gate="G$1" pin="HOLD" pad="64"/>
<connect gate="G$1" pin="INTR" pad="57"/>
<connect gate="G$1" pin="M/!IO" pad="67"/>
<connect gate="G$1" pin="NC@1" pad="2"/>
<connect gate="G$1" pin="NC@2" pad="3"/>
<connect gate="G$1" pin="NC@3" pad="55"/>
<connect gate="G$1" pin="NC@4" pad="56"/>
<connect gate="G$1" pin="NC@5" pad="58"/>
<connect gate="G$1" pin="NMI" pad="59"/>
<connect gate="G$1" pin="PEREQ" pad="61"/>
<connect gate="G$1" pin="RESET" pad="29"/>
<connect gate="P" pin="GND@1" pad="9"/>
<connect gate="P" pin="GND@2" pad="35"/>
<connect gate="P" pin="GND@3" pad="60"/>
<connect gate="P" pin="VCC@1" pad="30"/>
<connect gate="P" pin="VCC@2" pad="62"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8237-A" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8237-A"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="!IOR" pad="1"/>
<connect gate="G$1" pin="!IOW" pad="2"/>
<connect gate="G$1" pin="!MEMR" pad="3"/>
<connect gate="G$1" pin="!MEMW" pad="4"/>
<connect gate="G$1" pin="-" pad="5"/>
<connect gate="G$1" pin="A0" pad="32"/>
<connect gate="G$1" pin="A1" pad="33"/>
<connect gate="G$1" pin="A2" pad="34"/>
<connect gate="G$1" pin="A3" pad="35"/>
<connect gate="G$1" pin="A4" pad="37"/>
<connect gate="G$1" pin="A5" pad="38"/>
<connect gate="G$1" pin="A6" pad="39"/>
<connect gate="G$1" pin="A7" pad="40"/>
<connect gate="G$1" pin="ADSTB" pad="8"/>
<connect gate="G$1" pin="AEN" pad="9"/>
<connect gate="G$1" pin="CLK" pad="12"/>
<connect gate="G$1" pin="DACK0" pad="25"/>
<connect gate="G$1" pin="DACK1" pad="24"/>
<connect gate="G$1" pin="DACK2" pad="14"/>
<connect gate="G$1" pin="DACK3" pad="15"/>
<connect gate="G$1" pin="DB0" pad="30"/>
<connect gate="G$1" pin="DB1" pad="29"/>
<connect gate="G$1" pin="DB2" pad="28"/>
<connect gate="G$1" pin="DB3" pad="27"/>
<connect gate="G$1" pin="DB4" pad="26"/>
<connect gate="G$1" pin="DB5" pad="23"/>
<connect gate="G$1" pin="DB6" pad="22"/>
<connect gate="G$1" pin="DB7" pad="21"/>
<connect gate="G$1" pin="DREQ0" pad="19"/>
<connect gate="G$1" pin="DREQ1" pad="18"/>
<connect gate="G$1" pin="DREQ2" pad="17"/>
<connect gate="G$1" pin="DREQ3" pad="16"/>
<connect gate="G$1" pin="EOP" pad="36"/>
<connect gate="G$1" pin="HLDA" pad="7"/>
<connect gate="G$1" pin="HRQ" pad="10"/>
<connect gate="G$1" pin="READY" pad="6"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="VCC" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8237-B" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8237-B"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!CS" pad="11"/>
<connect gate="G$1" pin="!IOR" pad="1"/>
<connect gate="G$1" pin="!IOW" pad="2"/>
<connect gate="G$1" pin="!MEMR" pad="3"/>
<connect gate="G$1" pin="!MEMW" pad="4"/>
<connect gate="G$1" pin="A0" pad="32"/>
<connect gate="G$1" pin="A1" pad="33"/>
<connect gate="G$1" pin="A2" pad="34"/>
<connect gate="G$1" pin="A3" pad="35"/>
<connect gate="G$1" pin="A4" pad="37"/>
<connect gate="G$1" pin="A5" pad="38"/>
<connect gate="G$1" pin="A6" pad="39"/>
<connect gate="G$1" pin="A7" pad="40"/>
<connect gate="G$1" pin="ADSTB" pad="8"/>
<connect gate="G$1" pin="AEN" pad="9"/>
<connect gate="G$1" pin="CLK" pad="12"/>
<connect gate="G$1" pin="DACK0" pad="25"/>
<connect gate="G$1" pin="DACK1" pad="24"/>
<connect gate="G$1" pin="DACK2" pad="14"/>
<connect gate="G$1" pin="DACK3" pad="15"/>
<connect gate="G$1" pin="DB0" pad="30"/>
<connect gate="G$1" pin="DB1" pad="29"/>
<connect gate="G$1" pin="DB2" pad="28"/>
<connect gate="G$1" pin="DB3" pad="27"/>
<connect gate="G$1" pin="DB4" pad="26"/>
<connect gate="G$1" pin="DB5" pad="23"/>
<connect gate="G$1" pin="DB6" pad="22"/>
<connect gate="G$1" pin="DB7" pad="21"/>
<connect gate="G$1" pin="DREQ0" pad="19"/>
<connect gate="G$1" pin="DREQ1" pad="18"/>
<connect gate="G$1" pin="DREQ2" pad="17"/>
<connect gate="G$1" pin="DREQ3" pad="16"/>
<connect gate="G$1" pin="EOP" pad="36"/>
<connect gate="G$1" pin="HLDA" pad="7"/>
<connect gate="G$1" pin="HRQ" pad="10"/>
<connect gate="G$1" pin="MODE" pad="5"/>
<connect gate="G$1" pin="READY" pad="6"/>
<connect gate="G$1" pin="RESET" pad="13"/>
<connect gate="P" pin="GND" pad="20"/>
<connect gate="P" pin="VCC" pad="31"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82C59A-2" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82C59A-2"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!CS" pad="1"/>
<connect gate="G$1" pin="!INTA" pad="26"/>
<connect gate="G$1" pin="!RD" pad="3"/>
<connect gate="G$1" pin="!SP!/!EN" pad="16"/>
<connect gate="G$1" pin="!WR" pad="2"/>
<connect gate="G$1" pin="A0" pad="27"/>
<connect gate="G$1" pin="CAS0" pad="12"/>
<connect gate="G$1" pin="CAS1" pad="13"/>
<connect gate="G$1" pin="CAS2" pad="15"/>
<connect gate="G$1" pin="D0" pad="11"/>
<connect gate="G$1" pin="D1" pad="10"/>
<connect gate="G$1" pin="D2" pad="9"/>
<connect gate="G$1" pin="D3" pad="8"/>
<connect gate="G$1" pin="D4" pad="7"/>
<connect gate="G$1" pin="D5" pad="6"/>
<connect gate="G$1" pin="D6" pad="5"/>
<connect gate="G$1" pin="D7" pad="4"/>
<connect gate="G$1" pin="INT" pad="17"/>
<connect gate="G$1" pin="IR0" pad="18"/>
<connect gate="G$1" pin="IR1" pad="19"/>
<connect gate="G$1" pin="IR2" pad="20"/>
<connect gate="G$1" pin="IR3" pad="21"/>
<connect gate="G$1" pin="IR4" pad="22"/>
<connect gate="G$1" pin="IR5" pad="23"/>
<connect gate="G$1" pin="IR6" pad="24"/>
<connect gate="G$1" pin="IR7" pad="25"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CP82C59A-12Z"/>
<attribute name="OC_FARNELL" value="1561995"/>
<attribute name="OC_NEWARK" value="05M7148"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8282-A" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8282-A"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!OE" pad="9"/>
<connect gate="G$1" pin="DI0" pad="1"/>
<connect gate="G$1" pin="DI1" pad="2"/>
<connect gate="G$1" pin="DI2" pad="3"/>
<connect gate="G$1" pin="DI3" pad="4"/>
<connect gate="G$1" pin="DI4" pad="5"/>
<connect gate="G$1" pin="DI5" pad="6"/>
<connect gate="G$1" pin="DI6" pad="7"/>
<connect gate="G$1" pin="DI7" pad="8"/>
<connect gate="G$1" pin="DO0" pad="19"/>
<connect gate="G$1" pin="DO1" pad="18"/>
<connect gate="G$1" pin="DO2" pad="17"/>
<connect gate="G$1" pin="DO3" pad="16"/>
<connect gate="G$1" pin="DO4" pad="15"/>
<connect gate="G$1" pin="DO5" pad="14"/>
<connect gate="G$1" pin="DO6" pad="13"/>
<connect gate="G$1" pin="DO7" pad="12"/>
<connect gate="G$1" pin="STB" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8283-A" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8283-A"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!DO0" pad="19"/>
<connect gate="G$1" pin="!DO1" pad="18"/>
<connect gate="G$1" pin="!DO2" pad="17"/>
<connect gate="G$1" pin="!DO3" pad="16"/>
<connect gate="G$1" pin="!DO4" pad="15"/>
<connect gate="G$1" pin="!DO5" pad="14"/>
<connect gate="G$1" pin="!DO6" pad="13"/>
<connect gate="G$1" pin="!DO7" pad="12"/>
<connect gate="G$1" pin="!OE" pad="9"/>
<connect gate="G$1" pin="DI0" pad="1"/>
<connect gate="G$1" pin="DI1" pad="2"/>
<connect gate="G$1" pin="DI2" pad="3"/>
<connect gate="G$1" pin="DI3" pad="4"/>
<connect gate="G$1" pin="DI4" pad="5"/>
<connect gate="G$1" pin="DI5" pad="6"/>
<connect gate="G$1" pin="DI6" pad="7"/>
<connect gate="G$1" pin="DI7" pad="8"/>
<connect gate="G$1" pin="STB" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8284-B" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8284-B"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="!AEN1" pad="3"/>
<connect gate="G$1" pin="!AEN2" pad="7"/>
<connect gate="G$1" pin="!ASYNC" pad="15"/>
<connect gate="G$1" pin="!RES" pad="11"/>
<connect gate="G$1" pin="CLK" pad="8"/>
<connect gate="G$1" pin="CSYNC" pad="1"/>
<connect gate="G$1" pin="EFI" pad="14"/>
<connect gate="G$1" pin="F/!C" pad="13"/>
<connect gate="G$1" pin="OSC" pad="12"/>
<connect gate="G$1" pin="PCLK" pad="2"/>
<connect gate="G$1" pin="RDY1" pad="4"/>
<connect gate="G$1" pin="RDY2" pad="6"/>
<connect gate="G$1" pin="READY" pad="5"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="X1" pad="17"/>
<connect gate="G$1" pin="X2" pad="16"/>
<connect gate="P" pin="GND" pad="9"/>
<connect gate="P" pin="VCC" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8286-A" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8286-A"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!OE" pad="9"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="B0" pad="19"/>
<connect gate="G$1" pin="B1" pad="18"/>
<connect gate="G$1" pin="B2" pad="17"/>
<connect gate="G$1" pin="B3" pad="16"/>
<connect gate="G$1" pin="B4" pad="15"/>
<connect gate="G$1" pin="B5" pad="14"/>
<connect gate="G$1" pin="B6" pad="13"/>
<connect gate="G$1" pin="B7" pad="12"/>
<connect gate="G$1" pin="T" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8287-A" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8287-A"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!B0" pad="19"/>
<connect gate="G$1" pin="!B1" pad="18"/>
<connect gate="G$1" pin="!B2" pad="17"/>
<connect gate="G$1" pin="!B3" pad="16"/>
<connect gate="G$1" pin="!B4" pad="15"/>
<connect gate="G$1" pin="!B5" pad="14"/>
<connect gate="G$1" pin="!B6" pad="13"/>
<connect gate="G$1" pin="!B7" pad="12"/>
<connect gate="G$1" pin="!OE" pad="9"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="T" pad="11"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8288-A" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8288-A"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!AEN" pad="6"/>
<connect gate="G$1" pin="!AIOWC" pad="12"/>
<connect gate="G$1" pin="!AMWC" pad="8"/>
<connect gate="G$1" pin="!INTA" pad="14"/>
<connect gate="G$1" pin="!IORC" pad="13"/>
<connect gate="G$1" pin="!IOWC" pad="11"/>
<connect gate="G$1" pin="!MRDC" pad="7"/>
<connect gate="G$1" pin="!MWTC" pad="9"/>
<connect gate="G$1" pin="!S0" pad="19"/>
<connect gate="G$1" pin="!S1" pad="3"/>
<connect gate="G$1" pin="!S2" pad="18"/>
<connect gate="G$1" pin="ALE" pad="5"/>
<connect gate="G$1" pin="CEN" pad="15"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="DEN" pad="16"/>
<connect gate="G$1" pin="DT/!R" pad="4"/>
<connect gate="G$1" pin="IOB" pad="1"/>
<connect gate="G$1" pin="MCE/!PDEN" pad="17"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8289" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="8289"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!AEN" pad="13"/>
<connect gate="G$1" pin="!BCLK" pad="5"/>
<connect gate="G$1" pin="!BPRN" pad="9"/>
<connect gate="G$1" pin="!BPRO" pad="8"/>
<connect gate="G$1" pin="!BREQ" pad="7"/>
<connect gate="G$1" pin="!BUSY" pad="11"/>
<connect gate="G$1" pin="!CBRQ" pad="12"/>
<connect gate="G$1" pin="!CRQLCK" pad="15"/>
<connect gate="G$1" pin="!INIT" pad="6"/>
<connect gate="G$1" pin="!IOB" pad="2"/>
<connect gate="G$1" pin="!LOCK" pad="16"/>
<connect gate="G$1" pin="!S0" pad="18"/>
<connect gate="G$1" pin="!S1" pad="19"/>
<connect gate="G$1" pin="!S2" pad="1"/>
<connect gate="G$1" pin="ANYRQST" pad="14"/>
<connect gate="G$1" pin="CLK" pad="17"/>
<connect gate="G$1" pin="RESB" pad="4"/>
<connect gate="G$1" pin="SYSB/!RESB" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82200" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82200"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL22-3">
<connects>
<connect gate="G$1" pin="!CS" pad="16"/>
<connect gate="G$1" pin="!RD" pad="17"/>
<connect gate="G$1" pin="!WR" pad="18"/>
<connect gate="G$1" pin="A0" pad="19"/>
<connect gate="G$1" pin="A1" pad="20"/>
<connect gate="G$1" pin="ACK0" pad="2"/>
<connect gate="G$1" pin="ACK1" pad="4"/>
<connect gate="G$1" pin="ACK2" pad="6"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="D0" pad="15"/>
<connect gate="G$1" pin="D1" pad="14"/>
<connect gate="G$1" pin="D2" pad="13"/>
<connect gate="G$1" pin="D3" pad="12"/>
<connect gate="G$1" pin="FREQ" pad="7"/>
<connect gate="G$1" pin="INT/!DMA" pad="21"/>
<connect gate="G$1" pin="PACK" pad="8"/>
<connect gate="G$1" pin="REQ0" pad="1"/>
<connect gate="G$1" pin="REQ1" pad="3"/>
<connect gate="G$1" pin="REQ2" pad="5"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82C206" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82C206"/>
<gate name="P" symbol="2VCC3GND"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="G$1" pin="!ACK" pad="33"/>
<connect gate="G$1" pin="!AEN16" pad="64"/>
<connect gate="G$1" pin="!AEN8" pad="63"/>
<connect gate="G$1" pin="!DMAMEMR" pad="61"/>
<connect gate="G$1" pin="!DMAMEMW" pad="62"/>
<connect gate="G$1" pin="!INTA" pad="16"/>
<connect gate="G$1" pin="!PSRSTB" pad="15"/>
<connect gate="G$1" pin="!XIOR" pad="54"/>
<connect gate="G$1" pin="!XIOW" pad="52"/>
<connect gate="G$1" pin="A17" pad="11"/>
<connect gate="G$1" pin="A18" pad="10"/>
<connect gate="G$1" pin="A19" pad="9"/>
<connect gate="G$1" pin="A20" pad="8"/>
<connect gate="G$1" pin="A21" pad="7"/>
<connect gate="G$1" pin="A22" pad="6"/>
<connect gate="G$1" pin="A23" pad="5"/>
<connect gate="G$1" pin="ADSTB16" pad="65"/>
<connect gate="G$1" pin="ADSTB8" pad="66"/>
<connect gate="G$1" pin="AS" pad="71"/>
<connect gate="G$1" pin="DACK0" pad="48"/>
<connect gate="G$1" pin="DACK1" pad="49"/>
<connect gate="G$1" pin="DACK2" pad="50"/>
<connect gate="G$1" pin="DACK3" pad="51"/>
<connect gate="G$1" pin="DACK5" pad="57"/>
<connect gate="G$1" pin="DACK6" pad="56"/>
<connect gate="G$1" pin="DACK7" pad="55"/>
<connect gate="G$1" pin="DREQ0" pad="44"/>
<connect gate="G$1" pin="DREQ1" pad="45"/>
<connect gate="G$1" pin="DREQ2" pad="46"/>
<connect gate="G$1" pin="DREQ3" pad="47"/>
<connect gate="G$1" pin="DREQ5" pad="60"/>
<connect gate="G$1" pin="DREQ6" pad="59"/>
<connect gate="G$1" pin="DREQ7" pad="58"/>
<connect gate="G$1" pin="GATE2" pad="22"/>
<connect gate="G$1" pin="HLDA" pad="73"/>
<connect gate="G$1" pin="HRQ" pad="69"/>
<connect gate="G$1" pin="INTR" pad="70"/>
<connect gate="G$1" pin="IOCHRDY" pad="68"/>
<connect gate="G$1" pin="IRQ1" pad="4"/>
<connect gate="G$1" pin="IRQ10" pad="81"/>
<connect gate="G$1" pin="IRQ11" pad="80"/>
<connect gate="G$1" pin="IRQ12" pad="79"/>
<connect gate="G$1" pin="IRQ13" pad="78"/>
<connect gate="G$1" pin="IRQ14" pad="77"/>
<connect gate="G$1" pin="IRQ15" pad="76"/>
<connect gate="G$1" pin="IRQ3" pad="3"/>
<connect gate="G$1" pin="IRQ4" pad="2"/>
<connect gate="G$1" pin="IRQ5" pad="1"/>
<connect gate="G$1" pin="IRQ6" pad="84"/>
<connect gate="G$1" pin="IRQ7" pad="83"/>
<connect gate="G$1" pin="IRQ9" pad="82"/>
<connect gate="G$1" pin="OSCI" pad="72"/>
<connect gate="G$1" pin="OUT1" pad="20"/>
<connect gate="G$1" pin="OUT2" pad="19"/>
<connect gate="G$1" pin="PWRGD" pad="14"/>
<connect gate="G$1" pin="RESET" pad="18"/>
<connect gate="G$1" pin="SCLK" pad="21"/>
<connect gate="G$1" pin="TC" pad="67"/>
<connect gate="G$1" pin="TEST" pad="17"/>
<connect gate="G$1" pin="TMRCLK" pad="23"/>
<connect gate="G$1" pin="XA0" pad="43"/>
<connect gate="G$1" pin="XA1" pad="42"/>
<connect gate="G$1" pin="XA16" pad="13"/>
<connect gate="G$1" pin="XA2" pad="41"/>
<connect gate="G$1" pin="XA3" pad="40"/>
<connect gate="G$1" pin="XA4" pad="39"/>
<connect gate="G$1" pin="XA5" pad="38"/>
<connect gate="G$1" pin="XA6" pad="37"/>
<connect gate="G$1" pin="XA7" pad="36"/>
<connect gate="G$1" pin="XA8" pad="35"/>
<connect gate="G$1" pin="XA9" pad="34"/>
<connect gate="G$1" pin="XD0" pad="31"/>
<connect gate="G$1" pin="XD1" pad="30"/>
<connect gate="G$1" pin="XD2" pad="29"/>
<connect gate="G$1" pin="XD3" pad="28"/>
<connect gate="G$1" pin="XD4" pad="27"/>
<connect gate="G$1" pin="XD5" pad="26"/>
<connect gate="G$1" pin="XD6" pad="25"/>
<connect gate="G$1" pin="XD7" pad="24"/>
<connect gate="P" pin="GND@1" pad="12"/>
<connect gate="P" pin="GND@2" pad="53"/>
<connect gate="P" pin="GND@3" pad="74"/>
<connect gate="P" pin="VCC@1" pad="32"/>
<connect gate="P" pin="VCC@2" pad="75"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82220-1" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82220-1"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!DEN" pad="42"/>
<connect gate="G$1" pin="!PEX" pad="9"/>
<connect gate="G$1" pin="BMOD" pad="43"/>
<connect gate="G$1" pin="DIR0" pad="63"/>
<connect gate="G$1" pin="DIR1" pad="62"/>
<connect gate="G$1" pin="DIR2" pad="61"/>
<connect gate="G$1" pin="DX0" pad="10"/>
<connect gate="G$1" pin="DX1" pad="11"/>
<connect gate="G$1" pin="DX10" pad="21"/>
<connect gate="G$1" pin="DX11" pad="22"/>
<connect gate="G$1" pin="DX12" pad="23"/>
<connect gate="G$1" pin="DX13" pad="24"/>
<connect gate="G$1" pin="DX14" pad="25"/>
<connect gate="G$1" pin="DX15" pad="26"/>
<connect gate="G$1" pin="DX2" pad="12"/>
<connect gate="G$1" pin="DX3" pad="13"/>
<connect gate="G$1" pin="DX4" pad="14"/>
<connect gate="G$1" pin="DX5" pad="15"/>
<connect gate="G$1" pin="DX6" pad="16"/>
<connect gate="G$1" pin="DX7" pad="17"/>
<connect gate="G$1" pin="DX8" pad="19"/>
<connect gate="G$1" pin="DX9" pad="20"/>
<connect gate="G$1" pin="DY0" pad="31"/>
<connect gate="G$1" pin="DY1" pad="32"/>
<connect gate="G$1" pin="DY10" pad="44"/>
<connect gate="G$1" pin="DY11" pad="45"/>
<connect gate="G$1" pin="DY12" pad="46"/>
<connect gate="G$1" pin="DY13" pad="47"/>
<connect gate="G$1" pin="DY14" pad="48"/>
<connect gate="G$1" pin="DY15" pad="49"/>
<connect gate="G$1" pin="DY16/PY0" pad="50"/>
<connect gate="G$1" pin="DY17/PY1" pad="51"/>
<connect gate="G$1" pin="DY2" pad="33"/>
<connect gate="G$1" pin="DY3" pad="34"/>
<connect gate="G$1" pin="DY4" pad="36"/>
<connect gate="G$1" pin="DY5" pad="37"/>
<connect gate="G$1" pin="DY6" pad="38"/>
<connect gate="G$1" pin="DY7" pad="39"/>
<connect gate="G$1" pin="DY8" pad="40"/>
<connect gate="G$1" pin="DY9" pad="41"/>
<connect gate="G$1" pin="DZ0" pad="53"/>
<connect gate="G$1" pin="DZ1" pad="54"/>
<connect gate="G$1" pin="DZ10" pad="66"/>
<connect gate="G$1" pin="DZ11" pad="67"/>
<connect gate="G$1" pin="DZ12" pad="68"/>
<connect gate="G$1" pin="DZ13" pad="2"/>
<connect gate="G$1" pin="DZ14" pad="3"/>
<connect gate="G$1" pin="DZ15" pad="4"/>
<connect gate="G$1" pin="DZ16/PZ0" pad="5"/>
<connect gate="G$1" pin="DZ17/PZ1" pad="6"/>
<connect gate="G$1" pin="DZ2" pad="55"/>
<connect gate="G$1" pin="DZ3" pad="56"/>
<connect gate="G$1" pin="DZ4" pad="57"/>
<connect gate="G$1" pin="DZ5" pad="58"/>
<connect gate="G$1" pin="DZ6" pad="59"/>
<connect gate="G$1" pin="DZ7" pad="60"/>
<connect gate="G$1" pin="DZ8" pad="64"/>
<connect gate="G$1" pin="DZ9" pad="65"/>
<connect gate="G$1" pin="INVY" pad="7"/>
<connect gate="G$1" pin="PX0/DX16" pad="29"/>
<connect gate="G$1" pin="PX1/DX17" pad="30"/>
<connect gate="G$1" pin="STBX" pad="27"/>
<connect gate="G$1" pin="STBYZ" pad="28"/>
<connect gate="G$1" pin="SWAP" pad="8"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="52"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCC@2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82220-2" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82220-2"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!DEN" pad="42"/>
<connect gate="G$1" pin="!PEV" pad="9"/>
<connect gate="G$1" pin="BMOD" pad="43"/>
<connect gate="G$1" pin="DT/!R" pad="63"/>
<connect gate="G$1" pin="DV0" pad="10"/>
<connect gate="G$1" pin="DV1" pad="11"/>
<connect gate="G$1" pin="DV10" pad="21"/>
<connect gate="G$1" pin="DV11" pad="22"/>
<connect gate="G$1" pin="DV12" pad="23"/>
<connect gate="G$1" pin="DV13" pad="24"/>
<connect gate="G$1" pin="DV14" pad="25"/>
<connect gate="G$1" pin="DV15" pad="26"/>
<connect gate="G$1" pin="DV16" pad="53"/>
<connect gate="G$1" pin="DV17" pad="54"/>
<connect gate="G$1" pin="DV18" pad="55"/>
<connect gate="G$1" pin="DV19" pad="56"/>
<connect gate="G$1" pin="DV2" pad="12"/>
<connect gate="G$1" pin="DV20" pad="57"/>
<connect gate="G$1" pin="DV21" pad="58"/>
<connect gate="G$1" pin="DV22" pad="59"/>
<connect gate="G$1" pin="DV23" pad="60"/>
<connect gate="G$1" pin="DV24" pad="29"/>
<connect gate="G$1" pin="DV25" pad="30"/>
<connect gate="G$1" pin="DV26" pad="5"/>
<connect gate="G$1" pin="DV3" pad="13"/>
<connect gate="G$1" pin="DV4" pad="14"/>
<connect gate="G$1" pin="DV5" pad="15"/>
<connect gate="G$1" pin="DV6" pad="16"/>
<connect gate="G$1" pin="DV7" pad="17"/>
<connect gate="G$1" pin="DV8" pad="19"/>
<connect gate="G$1" pin="DV9" pad="20"/>
<connect gate="G$1" pin="DW0" pad="31"/>
<connect gate="G$1" pin="DW1" pad="32"/>
<connect gate="G$1" pin="DW10" pad="44"/>
<connect gate="G$1" pin="DW11" pad="45"/>
<connect gate="G$1" pin="DW12" pad="46"/>
<connect gate="G$1" pin="DW13" pad="47"/>
<connect gate="G$1" pin="DW14" pad="48"/>
<connect gate="G$1" pin="DW15" pad="49"/>
<connect gate="G$1" pin="DW16" pad="64"/>
<connect gate="G$1" pin="DW17" pad="65"/>
<connect gate="G$1" pin="DW18" pad="66"/>
<connect gate="G$1" pin="DW19" pad="67"/>
<connect gate="G$1" pin="DW2" pad="33"/>
<connect gate="G$1" pin="DW20" pad="68"/>
<connect gate="G$1" pin="DW21" pad="2"/>
<connect gate="G$1" pin="DW22" pad="3"/>
<connect gate="G$1" pin="DW23" pad="4"/>
<connect gate="G$1" pin="DW24" pad="50"/>
<connect gate="G$1" pin="DW25" pad="51"/>
<connect gate="G$1" pin="DW26" pad="6"/>
<connect gate="G$1" pin="DW3" pad="34"/>
<connect gate="G$1" pin="DW4" pad="36"/>
<connect gate="G$1" pin="DW5" pad="37"/>
<connect gate="G$1" pin="DW6" pad="38"/>
<connect gate="G$1" pin="DW7" pad="39"/>
<connect gate="G$1" pin="DW8" pad="40"/>
<connect gate="G$1" pin="DW9" pad="41"/>
<connect gate="G$1" pin="INVW" pad="7"/>
<connect gate="G$1" pin="STBV" pad="27"/>
<connect gate="G$1" pin="STBW" pad="28"/>
<connect gate="G$1" pin="SUBMOD0" pad="61"/>
<connect gate="G$1" pin="SUBMOD1" pad="62"/>
<connect gate="G$1" pin="SWAP" pad="8"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="52"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCC@2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82220-3" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82220-3"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!CCS" pad="5"/>
<connect gate="G$1" pin="!CS0" pad="29"/>
<connect gate="G$1" pin="!CS1" pad="30"/>
<connect gate="G$1" pin="!CS2" pad="50"/>
<connect gate="G$1" pin="!CS3" pad="51"/>
<connect gate="G$1" pin="!DEN" pad="42"/>
<connect gate="G$1" pin="!ENCS" pad="6"/>
<connect gate="G$1" pin="BMOD" pad="43"/>
<connect gate="G$1" pin="CSMOD0" pad="9"/>
<connect gate="G$1" pin="CSMOD1" pad="8"/>
<connect gate="G$1" pin="CSMOD2" pad="28"/>
<connect gate="G$1" pin="DT/!R" pad="63"/>
<connect gate="G$1" pin="DV0" pad="10"/>
<connect gate="G$1" pin="DV1" pad="11"/>
<connect gate="G$1" pin="DV10" pad="21"/>
<connect gate="G$1" pin="DV11" pad="22"/>
<connect gate="G$1" pin="DV12" pad="23"/>
<connect gate="G$1" pin="DV13" pad="24"/>
<connect gate="G$1" pin="DV14" pad="25"/>
<connect gate="G$1" pin="DV15" pad="26"/>
<connect gate="G$1" pin="DV16" pad="53"/>
<connect gate="G$1" pin="DV17" pad="54"/>
<connect gate="G$1" pin="DV18" pad="55"/>
<connect gate="G$1" pin="DV19" pad="56"/>
<connect gate="G$1" pin="DV2" pad="12"/>
<connect gate="G$1" pin="DV20" pad="57"/>
<connect gate="G$1" pin="DV21" pad="58"/>
<connect gate="G$1" pin="DV22" pad="59"/>
<connect gate="G$1" pin="DV23" pad="60"/>
<connect gate="G$1" pin="DV3" pad="13"/>
<connect gate="G$1" pin="DV4" pad="14"/>
<connect gate="G$1" pin="DV5" pad="15"/>
<connect gate="G$1" pin="DV6" pad="16"/>
<connect gate="G$1" pin="DV7" pad="17"/>
<connect gate="G$1" pin="DV8" pad="19"/>
<connect gate="G$1" pin="DV9" pad="20"/>
<connect gate="G$1" pin="DW0" pad="31"/>
<connect gate="G$1" pin="DW1" pad="32"/>
<connect gate="G$1" pin="DW10" pad="44"/>
<connect gate="G$1" pin="DW11" pad="45"/>
<connect gate="G$1" pin="DW12" pad="46"/>
<connect gate="G$1" pin="DW13" pad="47"/>
<connect gate="G$1" pin="DW14" pad="48"/>
<connect gate="G$1" pin="DW15" pad="49"/>
<connect gate="G$1" pin="DW16" pad="64"/>
<connect gate="G$1" pin="DW17" pad="65"/>
<connect gate="G$1" pin="DW18" pad="66"/>
<connect gate="G$1" pin="DW19" pad="67"/>
<connect gate="G$1" pin="DW2" pad="33"/>
<connect gate="G$1" pin="DW20" pad="68"/>
<connect gate="G$1" pin="DW21" pad="2"/>
<connect gate="G$1" pin="DW22" pad="3"/>
<connect gate="G$1" pin="DW23" pad="4"/>
<connect gate="G$1" pin="DW3" pad="34"/>
<connect gate="G$1" pin="DW4" pad="36"/>
<connect gate="G$1" pin="DW5" pad="37"/>
<connect gate="G$1" pin="DW6" pad="38"/>
<connect gate="G$1" pin="DW7" pad="39"/>
<connect gate="G$1" pin="DW8" pad="40"/>
<connect gate="G$1" pin="DW9" pad="41"/>
<connect gate="G$1" pin="INVW" pad="7"/>
<connect gate="G$1" pin="STB" pad="27"/>
<connect gate="G$1" pin="SUBMOD0" pad="61"/>
<connect gate="G$1" pin="SUBMOD1" pad="62"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="52"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCC@2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82220-4" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82220-4"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!AEN" pad="64"/>
<connect gate="G$1" pin="!DENIN" pad="42"/>
<connect gate="G$1" pin="!DENOUT" pad="6"/>
<connect gate="G$1" pin="!INTA" pad="2"/>
<connect gate="G$1" pin="!IORC" pad="67"/>
<connect gate="G$1" pin="!IOWC" pad="68"/>
<connect gate="G$1" pin="!MRDC" pad="65"/>
<connect gate="G$1" pin="!MWTC" pad="66"/>
<connect gate="G$1" pin="!PEV" pad="9"/>
<connect gate="G$1" pin="!READY" pad="58"/>
<connect gate="G$1" pin="!S0" pad="55"/>
<connect gate="G$1" pin="!S1" pad="56"/>
<connect gate="G$1" pin="!S2" pad="57"/>
<connect gate="G$1" pin="ALE" pad="4"/>
<connect gate="G$1" pin="BMOD" pad="43"/>
<connect gate="G$1" pin="CENL" pad="60"/>
<connect gate="G$1" pin="CLK" pad="54"/>
<connect gate="G$1" pin="CMDLY" pad="59"/>
<connect gate="G$1" pin="DT/!RIN" pad="63"/>
<connect gate="G$1" pin="DT/!ROUT" pad="5"/>
<connect gate="G$1" pin="DV0" pad="10"/>
<connect gate="G$1" pin="DV1" pad="11"/>
<connect gate="G$1" pin="DV10" pad="21"/>
<connect gate="G$1" pin="DV11" pad="22"/>
<connect gate="G$1" pin="DV12" pad="23"/>
<connect gate="G$1" pin="DV13" pad="24"/>
<connect gate="G$1" pin="DV14" pad="25"/>
<connect gate="G$1" pin="DV15" pad="26"/>
<connect gate="G$1" pin="DV16" pad="29"/>
<connect gate="G$1" pin="DV17" pad="30"/>
<connect gate="G$1" pin="DV2" pad="12"/>
<connect gate="G$1" pin="DV3" pad="13"/>
<connect gate="G$1" pin="DV4" pad="14"/>
<connect gate="G$1" pin="DV5" pad="15"/>
<connect gate="G$1" pin="DV6" pad="16"/>
<connect gate="G$1" pin="DV7" pad="17"/>
<connect gate="G$1" pin="DV8" pad="19"/>
<connect gate="G$1" pin="DV9" pad="20"/>
<connect gate="G$1" pin="DW0" pad="31"/>
<connect gate="G$1" pin="DW1" pad="32"/>
<connect gate="G$1" pin="DW10" pad="44"/>
<connect gate="G$1" pin="DW11" pad="45"/>
<connect gate="G$1" pin="DW12" pad="46"/>
<connect gate="G$1" pin="DW13" pad="47"/>
<connect gate="G$1" pin="DW14" pad="48"/>
<connect gate="G$1" pin="DW15" pad="49"/>
<connect gate="G$1" pin="DW16" pad="50"/>
<connect gate="G$1" pin="DW17" pad="51"/>
<connect gate="G$1" pin="DW2" pad="33"/>
<connect gate="G$1" pin="DW3" pad="34"/>
<connect gate="G$1" pin="DW4" pad="36"/>
<connect gate="G$1" pin="DW5" pad="37"/>
<connect gate="G$1" pin="DW6" pad="38"/>
<connect gate="G$1" pin="DW7" pad="39"/>
<connect gate="G$1" pin="DW8" pad="40"/>
<connect gate="G$1" pin="DW9" pad="41"/>
<connect gate="G$1" pin="INVW" pad="7"/>
<connect gate="G$1" pin="MB" pad="28"/>
<connect gate="G$1" pin="MCE" pad="3"/>
<connect gate="G$1" pin="MOD286" pad="53"/>
<connect gate="G$1" pin="STB" pad="27"/>
<connect gate="G$1" pin="SUBMOD0" pad="61"/>
<connect gate="G$1" pin="SUBMOD1" pad="62"/>
<connect gate="G$1" pin="SWAP" pad="8"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="52"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCC@2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82220-5" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82220-5"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!AEN" pad="64"/>
<connect gate="G$1" pin="!BCLK" pad="53"/>
<connect gate="G$1" pin="!BPRN" pad="27"/>
<connect gate="G$1" pin="!BPRO" pad="30"/>
<connect gate="G$1" pin="!BREQ" pad="29"/>
<connect gate="G$1" pin="!BUSY" pad="51"/>
<connect gate="G$1" pin="!CBQLCK" pad="50"/>
<connect gate="G$1" pin="!CBRQ" pad="5"/>
<connect gate="G$1" pin="!DENIN" pad="42"/>
<connect gate="G$1" pin="!INIT" pad="28"/>
<connect gate="G$1" pin="!INTA" pad="2"/>
<connect gate="G$1" pin="!IORC" pad="67"/>
<connect gate="G$1" pin="!IOWC" pad="68"/>
<connect gate="G$1" pin="!LLOCK" pad="6"/>
<connect gate="G$1" pin="!MRDC" pad="65"/>
<connect gate="G$1" pin="!MWTC" pad="66"/>
<connect gate="G$1" pin="!READY" pad="58"/>
<connect gate="G$1" pin="!S0" pad="55"/>
<connect gate="G$1" pin="!S1" pad="56"/>
<connect gate="G$1" pin="ALE" pad="4"/>
<connect gate="G$1" pin="BMOD" pad="43"/>
<connect gate="G$1" pin="CLK" pad="54"/>
<connect gate="G$1" pin="DT/!RIN" pad="63"/>
<connect gate="G$1" pin="DV0" pad="10"/>
<connect gate="G$1" pin="DV1" pad="11"/>
<connect gate="G$1" pin="DV10" pad="21"/>
<connect gate="G$1" pin="DV11" pad="22"/>
<connect gate="G$1" pin="DV12" pad="23"/>
<connect gate="G$1" pin="DV13" pad="24"/>
<connect gate="G$1" pin="DV14" pad="25"/>
<connect gate="G$1" pin="DV15" pad="26"/>
<connect gate="G$1" pin="DV2" pad="12"/>
<connect gate="G$1" pin="DV3" pad="13"/>
<connect gate="G$1" pin="DV4" pad="14"/>
<connect gate="G$1" pin="DV5" pad="15"/>
<connect gate="G$1" pin="DV6" pad="16"/>
<connect gate="G$1" pin="DV7" pad="17"/>
<connect gate="G$1" pin="DV8" pad="19"/>
<connect gate="G$1" pin="DV9" pad="20"/>
<connect gate="G$1" pin="DW0" pad="31"/>
<connect gate="G$1" pin="DW1" pad="32"/>
<connect gate="G$1" pin="DW10" pad="44"/>
<connect gate="G$1" pin="DW11" pad="45"/>
<connect gate="G$1" pin="DW12" pad="46"/>
<connect gate="G$1" pin="DW13" pad="47"/>
<connect gate="G$1" pin="DW14" pad="48"/>
<connect gate="G$1" pin="DW15" pad="49"/>
<connect gate="G$1" pin="DW2" pad="33"/>
<connect gate="G$1" pin="DW3" pad="34"/>
<connect gate="G$1" pin="DW4" pad="36"/>
<connect gate="G$1" pin="DW5" pad="37"/>
<connect gate="G$1" pin="DW6" pad="38"/>
<connect gate="G$1" pin="DW7" pad="39"/>
<connect gate="G$1" pin="DW8" pad="40"/>
<connect gate="G$1" pin="DW9" pad="41"/>
<connect gate="G$1" pin="INVW" pad="59"/>
<connect gate="G$1" pin="M/!IO" pad="57"/>
<connect gate="G$1" pin="MCE" pad="3"/>
<connect gate="G$1" pin="MODE" pad="7"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="SUBMOD0" pad="61"/>
<connect gate="G$1" pin="SUBMOD1" pad="62"/>
<connect gate="G$1" pin="SWAP" pad="8"/>
<connect gate="G$1" pin="SYSB" pad="60"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="52"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCC@2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82220-6" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82220-6"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!AEN" pad="28"/>
<connect gate="G$1" pin="!BHE" pad="50"/>
<connect gate="G$1" pin="!BHEN" pad="51"/>
<connect gate="G$1" pin="!DEN" pad="42"/>
<connect gate="G$1" pin="ALE" pad="27"/>
<connect gate="G$1" pin="BMOD" pad="43"/>
<connect gate="G$1" pin="DA0" pad="53"/>
<connect gate="G$1" pin="DA1" pad="54"/>
<connect gate="G$1" pin="DA10" pad="66"/>
<connect gate="G$1" pin="DA11" pad="67"/>
<connect gate="G$1" pin="DA12" pad="68"/>
<connect gate="G$1" pin="DA13" pad="2"/>
<connect gate="G$1" pin="DA14" pad="3"/>
<connect gate="G$1" pin="DA15" pad="4"/>
<connect gate="G$1" pin="DA16" pad="5"/>
<connect gate="G$1" pin="DA17" pad="6"/>
<connect gate="G$1" pin="DA2" pad="55"/>
<connect gate="G$1" pin="DA3" pad="56"/>
<connect gate="G$1" pin="DA4" pad="57"/>
<connect gate="G$1" pin="DA5" pad="58"/>
<connect gate="G$1" pin="DA6" pad="59"/>
<connect gate="G$1" pin="DA7" pad="60"/>
<connect gate="G$1" pin="DA8" pad="64"/>
<connect gate="G$1" pin="DA9" pad="65"/>
<connect gate="G$1" pin="DT/!R" pad="63"/>
<connect gate="G$1" pin="DX0" pad="10"/>
<connect gate="G$1" pin="DX1" pad="11"/>
<connect gate="G$1" pin="DX10" pad="21"/>
<connect gate="G$1" pin="DX11" pad="22"/>
<connect gate="G$1" pin="DX12" pad="23"/>
<connect gate="G$1" pin="DX13" pad="24"/>
<connect gate="G$1" pin="DX14" pad="25"/>
<connect gate="G$1" pin="DX15" pad="26"/>
<connect gate="G$1" pin="DX16" pad="29"/>
<connect gate="G$1" pin="DX17" pad="30"/>
<connect gate="G$1" pin="DX2" pad="12"/>
<connect gate="G$1" pin="DX3" pad="13"/>
<connect gate="G$1" pin="DX4" pad="14"/>
<connect gate="G$1" pin="DX5" pad="15"/>
<connect gate="G$1" pin="DX6" pad="16"/>
<connect gate="G$1" pin="DX7" pad="17"/>
<connect gate="G$1" pin="DX8" pad="19"/>
<connect gate="G$1" pin="DX9" pad="20"/>
<connect gate="G$1" pin="DY0" pad="31"/>
<connect gate="G$1" pin="DY1" pad="32"/>
<connect gate="G$1" pin="DY10" pad="44"/>
<connect gate="G$1" pin="DY11" pad="45"/>
<connect gate="G$1" pin="DY12" pad="46"/>
<connect gate="G$1" pin="DY13" pad="47"/>
<connect gate="G$1" pin="DY14" pad="48"/>
<connect gate="G$1" pin="DY15" pad="49"/>
<connect gate="G$1" pin="DY2" pad="33"/>
<connect gate="G$1" pin="DY3" pad="34"/>
<connect gate="G$1" pin="DY4" pad="36"/>
<connect gate="G$1" pin="DY5" pad="37"/>
<connect gate="G$1" pin="DY6" pad="38"/>
<connect gate="G$1" pin="DY7" pad="39"/>
<connect gate="G$1" pin="DY8" pad="40"/>
<connect gate="G$1" pin="DY9" pad="41"/>
<connect gate="G$1" pin="MODE" pad="7"/>
<connect gate="G$1" pin="RESET" pad="9"/>
<connect gate="G$1" pin="SUBMOD0" pad="61"/>
<connect gate="G$1" pin="SUBMOD1" pad="62"/>
<connect gate="G$1" pin="SWAPEN" pad="8"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="52"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCC@2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82257" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82257"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!BHE" pad="10"/>
<connect gate="G$1" pin="!CS" pad="17"/>
<connect gate="G$1" pin="!DACK0" pad="2"/>
<connect gate="G$1" pin="!DACK1" pad="3"/>
<connect gate="G$1" pin="!DACK2" pad="4"/>
<connect gate="G$1" pin="!DACK3" pad="5"/>
<connect gate="G$1" pin="!EOD0" pad="6"/>
<connect gate="G$1" pin="!EOD1" pad="7"/>
<connect gate="G$1" pin="!EOD2" pad="8"/>
<connect gate="G$1" pin="!EOD3" pad="9"/>
<connect gate="G$1" pin="!RD" pad="11"/>
<connect gate="G$1" pin="!READY" pad="19"/>
<connect gate="G$1" pin="!S0" pad="22"/>
<connect gate="G$1" pin="!S1" pad="20"/>
<connect gate="G$1" pin="!WR" pad="12"/>
<connect gate="G$1" pin="A0" pad="44"/>
<connect gate="G$1" pin="A1" pad="45"/>
<connect gate="G$1" pin="A10" pad="55"/>
<connect gate="G$1" pin="A11" pad="56"/>
<connect gate="G$1" pin="A12" pad="57"/>
<connect gate="G$1" pin="A13" pad="58"/>
<connect gate="G$1" pin="A14" pad="59"/>
<connect gate="G$1" pin="A15" pad="60"/>
<connect gate="G$1" pin="A16" pad="61"/>
<connect gate="G$1" pin="A17" pad="62"/>
<connect gate="G$1" pin="A18" pad="63"/>
<connect gate="G$1" pin="A19" pad="64"/>
<connect gate="G$1" pin="A2" pad="46"/>
<connect gate="G$1" pin="A20" pad="65"/>
<connect gate="G$1" pin="A21" pad="66"/>
<connect gate="G$1" pin="A22" pad="67"/>
<connect gate="G$1" pin="A23" pad="68"/>
<connect gate="G$1" pin="A3" pad="47"/>
<connect gate="G$1" pin="A4" pad="48"/>
<connect gate="G$1" pin="A5" pad="49"/>
<connect gate="G$1" pin="A6" pad="50"/>
<connect gate="G$1" pin="A7" pad="51"/>
<connect gate="G$1" pin="A8" pad="53"/>
<connect gate="G$1" pin="A9" pad="54"/>
<connect gate="G$1" pin="CLK" pad="21"/>
<connect gate="G$1" pin="D0" pad="43"/>
<connect gate="G$1" pin="D1" pad="41"/>
<connect gate="G$1" pin="D10" pad="38"/>
<connect gate="G$1" pin="D11" pad="36"/>
<connect gate="G$1" pin="D12" pad="33"/>
<connect gate="G$1" pin="D13" pad="31"/>
<connect gate="G$1" pin="D14" pad="29"/>
<connect gate="G$1" pin="D15" pad="27"/>
<connect gate="G$1" pin="D2" pad="39"/>
<connect gate="G$1" pin="D3" pad="37"/>
<connect gate="G$1" pin="D4" pad="34"/>
<connect gate="G$1" pin="D5" pad="32"/>
<connect gate="G$1" pin="D6" pad="30"/>
<connect gate="G$1" pin="D7" pad="28"/>
<connect gate="G$1" pin="D8" pad="42"/>
<connect gate="G$1" pin="D9" pad="40"/>
<connect gate="G$1" pin="DREQ0" pad="16"/>
<connect gate="G$1" pin="DREQ1" pad="15"/>
<connect gate="G$1" pin="DREQ2" pad="14"/>
<connect gate="G$1" pin="DREQ3" pad="13"/>
<connect gate="G$1" pin="HLDA" pad="26"/>
<connect gate="G$1" pin="HOLD" pad="25"/>
<connect gate="G$1" pin="M/!IO" pad="23"/>
<connect gate="G$1" pin="RESET" pad="24"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="52"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCC@2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82258" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82258"/>
<gate name="P" symbol="2VCC2GND"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="!BHE" pad="10"/>
<connect gate="G$1" pin="!CS" pad="17"/>
<connect gate="G$1" pin="!DACK0" pad="2"/>
<connect gate="G$1" pin="!DACK1" pad="3"/>
<connect gate="G$1" pin="!DACK2" pad="4"/>
<connect gate="G$1" pin="!DACK3" pad="5"/>
<connect gate="G$1" pin="!EOD0" pad="6"/>
<connect gate="G$1" pin="!EOD1" pad="7"/>
<connect gate="G$1" pin="!EOD2" pad="8"/>
<connect gate="G$1" pin="!EOD3" pad="9"/>
<connect gate="G$1" pin="!RD" pad="11"/>
<connect gate="G$1" pin="!READY" pad="19"/>
<connect gate="G$1" pin="!S0" pad="22"/>
<connect gate="G$1" pin="!S1" pad="20"/>
<connect gate="G$1" pin="!WR" pad="12"/>
<connect gate="G$1" pin="A0" pad="44"/>
<connect gate="G$1" pin="A1" pad="45"/>
<connect gate="G$1" pin="A10" pad="55"/>
<connect gate="G$1" pin="A11" pad="56"/>
<connect gate="G$1" pin="A12" pad="57"/>
<connect gate="G$1" pin="A13" pad="58"/>
<connect gate="G$1" pin="A14" pad="59"/>
<connect gate="G$1" pin="A15" pad="60"/>
<connect gate="G$1" pin="A16" pad="61"/>
<connect gate="G$1" pin="A17" pad="62"/>
<connect gate="G$1" pin="A18" pad="63"/>
<connect gate="G$1" pin="A19" pad="64"/>
<connect gate="G$1" pin="A2" pad="46"/>
<connect gate="G$1" pin="A20" pad="65"/>
<connect gate="G$1" pin="A21" pad="66"/>
<connect gate="G$1" pin="A22" pad="67"/>
<connect gate="G$1" pin="A23" pad="68"/>
<connect gate="G$1" pin="A3" pad="47"/>
<connect gate="G$1" pin="A4" pad="48"/>
<connect gate="G$1" pin="A5" pad="49"/>
<connect gate="G$1" pin="A6" pad="50"/>
<connect gate="G$1" pin="A7" pad="51"/>
<connect gate="G$1" pin="A8" pad="53"/>
<connect gate="G$1" pin="A9" pad="54"/>
<connect gate="G$1" pin="CLK" pad="21"/>
<connect gate="G$1" pin="D0" pad="43"/>
<connect gate="G$1" pin="D1" pad="41"/>
<connect gate="G$1" pin="D10" pad="38"/>
<connect gate="G$1" pin="D11" pad="36"/>
<connect gate="G$1" pin="D12" pad="33"/>
<connect gate="G$1" pin="D13" pad="31"/>
<connect gate="G$1" pin="D14" pad="29"/>
<connect gate="G$1" pin="D15" pad="27"/>
<connect gate="G$1" pin="D2" pad="39"/>
<connect gate="G$1" pin="D3" pad="37"/>
<connect gate="G$1" pin="D4" pad="34"/>
<connect gate="G$1" pin="D5" pad="32"/>
<connect gate="G$1" pin="D6" pad="30"/>
<connect gate="G$1" pin="D7" pad="28"/>
<connect gate="G$1" pin="D8" pad="42"/>
<connect gate="G$1" pin="D9" pad="40"/>
<connect gate="G$1" pin="DREQ0" pad="16"/>
<connect gate="G$1" pin="DREQ1" pad="15"/>
<connect gate="G$1" pin="DREQ2" pad="14"/>
<connect gate="G$1" pin="DREQ3" pad="13"/>
<connect gate="G$1" pin="HLDA" pad="26"/>
<connect gate="G$1" pin="HOLD" pad="25"/>
<connect gate="G$1" pin="M/!IO" pad="23"/>
<connect gate="G$1" pin="RESET" pad="24"/>
<connect gate="P" pin="GND@1" pad="18"/>
<connect gate="P" pin="GND@2" pad="52"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCC@2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82284" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82284"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="!ARDY" pad="1"/>
<connect gate="G$1" pin="!ARDYEN" pad="17"/>
<connect gate="G$1" pin="!READY" pad="4"/>
<connect gate="G$1" pin="!RES" pad="11"/>
<connect gate="G$1" pin="!S0" pad="15"/>
<connect gate="G$1" pin="!S1" pad="16"/>
<connect gate="G$1" pin="!SRDY" pad="2"/>
<connect gate="G$1" pin="!SRDYEN" pad="3"/>
<connect gate="G$1" pin="CLK" pad="10"/>
<connect gate="G$1" pin="EFI" pad="5"/>
<connect gate="G$1" pin="F/!C" pad="6"/>
<connect gate="G$1" pin="NC" pad="14"/>
<connect gate="G$1" pin="PCLK" pad="13"/>
<connect gate="G$1" pin="RESET" pad="12"/>
<connect gate="G$1" pin="X1" pad="7"/>
<connect gate="G$1" pin="X2" pad="8"/>
<connect gate="P" pin="GND" pad="9"/>
<connect gate="P" pin="VCC" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82288" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82288"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!INTA" pad="13"/>
<connect gate="G$1" pin="!IORC" pad="12"/>
<connect gate="G$1" pin="!IOWC" pad="11"/>
<connect gate="G$1" pin="!MRDC" pad="8"/>
<connect gate="G$1" pin="!MWTC" pad="9"/>
<connect gate="G$1" pin="!READY" pad="1"/>
<connect gate="G$1" pin="!S0" pad="19"/>
<connect gate="G$1" pin="!S1" pad="3"/>
<connect gate="G$1" pin="ALE" pad="5"/>
<connect gate="G$1" pin="CEN" pad="15"/>
<connect gate="G$1" pin="CENL" pad="14"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="CMDLY" pad="7"/>
<connect gate="G$1" pin="DEN" pad="16"/>
<connect gate="G$1" pin="DT/!R" pad="17"/>
<connect gate="G$1" pin="M/!IO" pad="18"/>
<connect gate="G$1" pin="MB" pad="6"/>
<connect gate="G$1" pin="MCE" pad="4"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82289" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82289"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="G$1" pin="!AEN" pad="13"/>
<connect gate="G$1" pin="!ALWAYS" pad="15"/>
<connect gate="G$1" pin="!BCLK" pad="5"/>
<connect gate="G$1" pin="!BPRN" pad="9"/>
<connect gate="G$1" pin="!BPRO" pad="8"/>
<connect gate="G$1" pin="!BREQ" pad="7"/>
<connect gate="G$1" pin="!BUSY" pad="11"/>
<connect gate="G$1" pin="!CBRQ" pad="12"/>
<connect gate="G$1" pin="!INIT" pad="6"/>
<connect gate="G$1" pin="!LLOCK" pad="14"/>
<connect gate="G$1" pin="!LOCK" pad="16"/>
<connect gate="G$1" pin="!READY" pad="2"/>
<connect gate="G$1" pin="!S0" pad="18"/>
<connect gate="G$1" pin="!S1" pad="19"/>
<connect gate="G$1" pin="CLK" pad="17"/>
<connect gate="G$1" pin="M/!IO" pad="1"/>
<connect gate="G$1" pin="RESET" pad="4"/>
<connect gate="G$1" pin="SYSB" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="VCC" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="82532" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="82532"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="ALE" pad="9"/>
<connect gate="G$1" pin="BHE" pad="10"/>
<connect gate="G$1" pin="CDA" pad="42"/>
<connect gate="G$1" pin="CDB" pad="41"/>
<connect gate="G$1" pin="CS" pad="13"/>
<connect gate="G$1" pin="CTSA" pad="16"/>
<connect gate="G$1" pin="CTSB" pad="19"/>
<connect gate="G$1" pin="D0" pad="60"/>
<connect gate="G$1" pin="D1" pad="59"/>
<connect gate="G$1" pin="D10" pad="50"/>
<connect gate="G$1" pin="D11" pad="49"/>
<connect gate="G$1" pin="D12" pad="48"/>
<connect gate="G$1" pin="D13" pad="47"/>
<connect gate="G$1" pin="D14" pad="46"/>
<connect gate="G$1" pin="D15" pad="45"/>
<connect gate="G$1" pin="D2" pad="58"/>
<connect gate="G$1" pin="D3" pad="57"/>
<connect gate="G$1" pin="D4" pad="56"/>
<connect gate="G$1" pin="D5" pad="55"/>
<connect gate="G$1" pin="D6" pad="54"/>
<connect gate="G$1" pin="D7" pad="53"/>
<connect gate="G$1" pin="D8" pad="52"/>
<connect gate="G$1" pin="D9" pad="51"/>
<connect gate="G$1" pin="DACKA" pad="36"/>
<connect gate="G$1" pin="DACKB" pad="35"/>
<connect gate="G$1" pin="DRRA" pad="32"/>
<connect gate="G$1" pin="DRRB" pad="31"/>
<connect gate="G$1" pin="DRTA" pad="34"/>
<connect gate="G$1" pin="DRTB" pad="33"/>
<connect gate="G$1" pin="DTACK" pad="22"/>
<connect gate="G$1" pin="GND" pad="30"/>
<connect gate="G$1" pin="GND@1" pad="61"/>
<connect gate="G$1" pin="IE0" pad="24"/>
<connect gate="G$1" pin="IE1" pad="23"/>
<connect gate="G$1" pin="INT" pad="26"/>
<connect gate="G$1" pin="INTA" pad="25"/>
<connect gate="G$1" pin="P00" pad="62"/>
<connect gate="G$1" pin="P01" pad="63"/>
<connect gate="G$1" pin="P02" pad="64"/>
<connect gate="G$1" pin="P03" pad="65"/>
<connect gate="G$1" pin="P04" pad="66"/>
<connect gate="G$1" pin="P05" pad="67"/>
<connect gate="G$1" pin="P06" pad="68"/>
<connect gate="G$1" pin="P07" pad="1"/>
<connect gate="G$1" pin="RD" pad="11"/>
<connect gate="G$1" pin="RESET" pad="28"/>
<connect gate="G$1" pin="RTSA" pad="15"/>
<connect gate="G$1" pin="RTSB" pad="20"/>
<connect gate="G$1" pin="RXCLKA" pad="43"/>
<connect gate="G$1" pin="RXCLKB" pad="40"/>
<connect gate="G$1" pin="RXDA" pad="14"/>
<connect gate="G$1" pin="RXDB" pad="21"/>
<connect gate="G$1" pin="TXCLKA" pad="44"/>
<connect gate="G$1" pin="TXCLKB" pad="39"/>
<connect gate="G$1" pin="TXDA" pad="17"/>
<connect gate="G$1" pin="TXDB" pad="18"/>
<connect gate="G$1" pin="VCC" pad="27"/>
<connect gate="G$1" pin="WITH" pad="29"/>
<connect gate="G$1" pin="WR" pad="12"/>
<connect gate="G$1" pin="XTAL1" pad="38"/>
<connect gate="G$1" pin="XTAL2" pad="37"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTS711" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="BTS711"/>
<gate name="B" symbol="BTS711"/>
<gate name="P" symbol="+VBB"/>
</gates>
<devices>
<device name="" package="PDSO_20-9">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN1" pad="3"/>
<connect gate="A" pin="IN2" pad="5"/>
<connect gate="A" pin="OUT1" pad="18"/>
<connect gate="A" pin="OUT2" pad="17"/>
<connect gate="A" pin="ST1/2" pad="4"/>
<connect gate="B" pin="GND" pad="6"/>
<connect gate="B" pin="IN1" pad="7"/>
<connect gate="B" pin="IN2" pad="9"/>
<connect gate="B" pin="OUT1" pad="14"/>
<connect gate="B" pin="OUT2" pad="13"/>
<connect gate="B" pin="ST1/2" pad="8"/>
<connect gate="P" pin="+VBB@1" pad="1"/>
<connect gate="P" pin="+VBB@2" pad="10"/>
<connect gate="P" pin="+VBB@3" pad="11"/>
<connect gate="P" pin="+VBB@4" pad="12"/>
<connect gate="P" pin="+VBB@5" pad="15"/>
<connect gate="P" pin="+VBB@6" pad="16"/>
<connect gate="P" pin="+VBB@7" pad="19"/>
<connect gate="P" pin="+VBB@8" pad="20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="BTS711L1."/>
<attribute name="OC_FARNELL" value="743380"/>
<attribute name="OC_NEWARK" value="46WX1412"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="80C535" prefix="IC">
<description>&lt;b&gt;80C515/80C535  8-Bit CMOS Single-Chip Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/cmc_upload/migrated_files/document_files/Datasheet/d80515.pdf</description>
<gates>
<gate name="G$1" symbol="80C535"/>
<gate name="P" symbol="2VCC1GND"/>
</gates>
<devices>
<device name="M" package="MQFP80-1">
<connects>
<connect gate="G$1" pin="ALE" pad="48"/>
<connect gate="G$1" pin="CLKOUTP1.6" pad="25"/>
<connect gate="G$1" pin="EA" pad="49"/>
<connect gate="G$1" pin="INT2/P1.4" pad="27"/>
<connect gate="G$1" pin="INT3/P1.0" pad="31"/>
<connect gate="G$1" pin="INT4/P1.1" pad="30"/>
<connect gate="G$1" pin="INT5/P1.2" pad="29"/>
<connect gate="G$1" pin="INT6/P1.3" pad="28"/>
<connect gate="G$1" pin="P0.0" pad="52"/>
<connect gate="G$1" pin="P0.1" pad="53"/>
<connect gate="G$1" pin="P0.2" pad="54"/>
<connect gate="G$1" pin="P0.3" pad="55"/>
<connect gate="G$1" pin="P0.4" pad="56"/>
<connect gate="G$1" pin="P0.5" pad="57"/>
<connect gate="G$1" pin="P0.6" pad="58"/>
<connect gate="G$1" pin="P0.7" pad="59"/>
<connect gate="G$1" pin="P2.0" pad="38"/>
<connect gate="G$1" pin="P2.1" pad="39"/>
<connect gate="G$1" pin="P2.2" pad="40"/>
<connect gate="G$1" pin="P2.3" pad="41"/>
<connect gate="G$1" pin="P2.4" pad="42"/>
<connect gate="G$1" pin="P2.5" pad="43"/>
<connect gate="G$1" pin="P2.6" pad="44"/>
<connect gate="G$1" pin="P2.7" pad="45"/>
<connect gate="G$1" pin="P3.0" pad="15"/>
<connect gate="G$1" pin="P3.1" pad="16"/>
<connect gate="G$1" pin="P3.2" pad="17"/>
<connect gate="G$1" pin="P3.3" pad="18"/>
<connect gate="G$1" pin="P3.4/T0" pad="19"/>
<connect gate="G$1" pin="P3.5/T1" pad="20"/>
<connect gate="G$1" pin="P3.6/WR" pad="21"/>
<connect gate="G$1" pin="P3.7/RD" pad="22"/>
<connect gate="G$1" pin="P4.0" pad="72"/>
<connect gate="G$1" pin="P4.1" pad="73"/>
<connect gate="G$1" pin="P4.2" pad="74"/>
<connect gate="G$1" pin="P4.3" pad="76"/>
<connect gate="G$1" pin="P4.4" pad="77"/>
<connect gate="G$1" pin="P4.5" pad="78"/>
<connect gate="G$1" pin="P4.6" pad="79"/>
<connect gate="G$1" pin="P4.7" pad="80"/>
<connect gate="G$1" pin="P5.0" pad="67"/>
<connect gate="G$1" pin="P5.1" pad="66"/>
<connect gate="G$1" pin="P5.2" pad="65"/>
<connect gate="G$1" pin="P5.3" pad="64"/>
<connect gate="G$1" pin="P5.4" pad="63"/>
<connect gate="G$1" pin="P5.5" pad="62"/>
<connect gate="G$1" pin="P5.6" pad="61"/>
<connect gate="G$1" pin="P5.7" pad="60"/>
<connect gate="G$1" pin="P6.0" pad="12"/>
<connect gate="G$1" pin="P6.1" pad="11"/>
<connect gate="G$1" pin="P6.2" pad="10"/>
<connect gate="G$1" pin="P6.3" pad="9"/>
<connect gate="G$1" pin="P6.4" pad="8"/>
<connect gate="G$1" pin="P6.5" pad="7"/>
<connect gate="G$1" pin="P6.6" pad="6"/>
<connect gate="G$1" pin="P6.7" pad="5"/>
<connect gate="G$1" pin="PE" pad="75"/>
<connect gate="G$1" pin="PSEN" pad="47"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="T2/P1.7" pad="24"/>
<connect gate="G$1" pin="T2EX/P1.5" pad="26"/>
<connect gate="G$1" pin="VAGND" pad="4"/>
<connect gate="G$1" pin="VAREF" pad="3"/>
<connect gate="G$1" pin="XTAL1" pad="37"/>
<connect gate="G$1" pin="XTAL2" pad="36"/>
<connect gate="P" pin="GND@1" pad="34"/>
<connect gate="P" pin="VCC@1" pad="33"/>
<connect gate="P" pin="VCC@2" pad="69"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N" package="PLCC68">
<connects>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="CLKOUTP1.6" pad="30"/>
<connect gate="G$1" pin="EA" pad="51"/>
<connect gate="G$1" pin="INT2/P1.4" pad="32"/>
<connect gate="G$1" pin="INT3/P1.0" pad="36"/>
<connect gate="G$1" pin="INT4/P1.1" pad="35"/>
<connect gate="G$1" pin="INT5/P1.2" pad="34"/>
<connect gate="G$1" pin="INT6/P1.3" pad="33"/>
<connect gate="G$1" pin="P0.0" pad="52"/>
<connect gate="G$1" pin="P0.1" pad="53"/>
<connect gate="G$1" pin="P0.2" pad="54"/>
<connect gate="G$1" pin="P0.3" pad="55"/>
<connect gate="G$1" pin="P0.4" pad="56"/>
<connect gate="G$1" pin="P0.5" pad="57"/>
<connect gate="G$1" pin="P0.6" pad="58"/>
<connect gate="G$1" pin="P0.7" pad="59"/>
<connect gate="G$1" pin="P2.0" pad="41"/>
<connect gate="G$1" pin="P2.1" pad="42"/>
<connect gate="G$1" pin="P2.2" pad="43"/>
<connect gate="G$1" pin="P2.3" pad="44"/>
<connect gate="G$1" pin="P2.4" pad="45"/>
<connect gate="G$1" pin="P2.5" pad="46"/>
<connect gate="G$1" pin="P2.6" pad="47"/>
<connect gate="G$1" pin="P2.7" pad="48"/>
<connect gate="G$1" pin="P3.0" pad="21"/>
<connect gate="G$1" pin="P3.1" pad="22"/>
<connect gate="G$1" pin="P3.2" pad="23"/>
<connect gate="G$1" pin="P3.3" pad="24"/>
<connect gate="G$1" pin="P3.4/T0" pad="25"/>
<connect gate="G$1" pin="P3.5/T1" pad="26"/>
<connect gate="G$1" pin="P3.6/WR" pad="27"/>
<connect gate="G$1" pin="P3.7/RD" pad="28"/>
<connect gate="G$1" pin="P4.0" pad="1"/>
<connect gate="G$1" pin="P4.1" pad="2"/>
<connect gate="G$1" pin="P4.2" pad="3"/>
<connect gate="G$1" pin="P4.3" pad="5"/>
<connect gate="G$1" pin="P4.4" pad="6"/>
<connect gate="G$1" pin="P4.5" pad="7"/>
<connect gate="G$1" pin="P4.6" pad="8"/>
<connect gate="G$1" pin="P4.7" pad="9"/>
<connect gate="G$1" pin="P5.0" pad="67"/>
<connect gate="G$1" pin="P5.1" pad="66"/>
<connect gate="G$1" pin="P5.2" pad="65"/>
<connect gate="G$1" pin="P5.3" pad="64"/>
<connect gate="G$1" pin="P5.4" pad="63"/>
<connect gate="G$1" pin="P5.5" pad="62"/>
<connect gate="G$1" pin="P5.6" pad="61"/>
<connect gate="G$1" pin="P5.7" pad="60"/>
<connect gate="G$1" pin="P6.0" pad="20"/>
<connect gate="G$1" pin="P6.1" pad="19"/>
<connect gate="G$1" pin="P6.2" pad="18"/>
<connect gate="G$1" pin="P6.3" pad="17"/>
<connect gate="G$1" pin="P6.4" pad="16"/>
<connect gate="G$1" pin="P6.5" pad="15"/>
<connect gate="G$1" pin="P6.6" pad="14"/>
<connect gate="G$1" pin="P6.7" pad="13"/>
<connect gate="G$1" pin="PE" pad="4"/>
<connect gate="G$1" pin="PSEN" pad="49"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="T2/P1.7" pad="29"/>
<connect gate="G$1" pin="T2EX/P1.5" pad="31"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="GND@1" pad="38"/>
<connect gate="P" pin="VCC@1" pad="37"/>
<connect gate="P" pin="VCC@2" pad="68"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N-S" package="PLCC68SOCK">
<connects>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="CLKOUTP1.6" pad="30"/>
<connect gate="G$1" pin="EA" pad="51"/>
<connect gate="G$1" pin="INT2/P1.4" pad="32"/>
<connect gate="G$1" pin="INT3/P1.0" pad="36"/>
<connect gate="G$1" pin="INT4/P1.1" pad="35"/>
<connect gate="G$1" pin="INT5/P1.2" pad="34"/>
<connect gate="G$1" pin="INT6/P1.3" pad="33"/>
<connect gate="G$1" pin="P0.0" pad="52"/>
<connect gate="G$1" pin="P0.1" pad="53"/>
<connect gate="G$1" pin="P0.2" pad="54"/>
<connect gate="G$1" pin="P0.3" pad="55"/>
<connect gate="G$1" pin="P0.4" pad="56"/>
<connect gate="G$1" pin="P0.5" pad="57"/>
<connect gate="G$1" pin="P0.6" pad="58"/>
<connect gate="G$1" pin="P0.7" pad="59"/>
<connect gate="G$1" pin="P2.0" pad="41"/>
<connect gate="G$1" pin="P2.1" pad="42"/>
<connect gate="G$1" pin="P2.2" pad="43"/>
<connect gate="G$1" pin="P2.3" pad="44"/>
<connect gate="G$1" pin="P2.4" pad="45"/>
<connect gate="G$1" pin="P2.5" pad="46"/>
<connect gate="G$1" pin="P2.6" pad="47"/>
<connect gate="G$1" pin="P2.7" pad="48"/>
<connect gate="G$1" pin="P3.0" pad="21"/>
<connect gate="G$1" pin="P3.1" pad="22"/>
<connect gate="G$1" pin="P3.2" pad="23"/>
<connect gate="G$1" pin="P3.3" pad="24"/>
<connect gate="G$1" pin="P3.4/T0" pad="25"/>
<connect gate="G$1" pin="P3.5/T1" pad="26"/>
<connect gate="G$1" pin="P3.6/WR" pad="27"/>
<connect gate="G$1" pin="P3.7/RD" pad="28"/>
<connect gate="G$1" pin="P4.0" pad="1"/>
<connect gate="G$1" pin="P4.1" pad="2"/>
<connect gate="G$1" pin="P4.2" pad="3"/>
<connect gate="G$1" pin="P4.3" pad="5"/>
<connect gate="G$1" pin="P4.4" pad="6"/>
<connect gate="G$1" pin="P4.5" pad="7"/>
<connect gate="G$1" pin="P4.6" pad="8"/>
<connect gate="G$1" pin="P4.7" pad="9"/>
<connect gate="G$1" pin="P5.0" pad="67"/>
<connect gate="G$1" pin="P5.1" pad="66"/>
<connect gate="G$1" pin="P5.2" pad="65"/>
<connect gate="G$1" pin="P5.3" pad="64"/>
<connect gate="G$1" pin="P5.4" pad="63"/>
<connect gate="G$1" pin="P5.5" pad="62"/>
<connect gate="G$1" pin="P5.6" pad="61"/>
<connect gate="G$1" pin="P5.7" pad="60"/>
<connect gate="G$1" pin="P6.0" pad="20"/>
<connect gate="G$1" pin="P6.1" pad="19"/>
<connect gate="G$1" pin="P6.2" pad="18"/>
<connect gate="G$1" pin="P6.3" pad="17"/>
<connect gate="G$1" pin="P6.4" pad="16"/>
<connect gate="G$1" pin="P6.5" pad="15"/>
<connect gate="G$1" pin="P6.6" pad="14"/>
<connect gate="G$1" pin="P6.7" pad="13"/>
<connect gate="G$1" pin="PE" pad="4"/>
<connect gate="G$1" pin="PSEN" pad="49"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="T2/P1.7" pad="29"/>
<connect gate="G$1" pin="T2EX/P1.5" pad="31"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="GND@1" pad="38"/>
<connect gate="P" pin="VCC@1" pad="37"/>
<connect gate="P" pin="VCC@2" pad="68"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DPC31" prefix="IC">
<description>&lt;b&gt;DPC31 Siemens PROFIBUS-DP Controller mit C31 Core&lt;/bv&gt;&lt;p&gt;
Suurce: dpc31_d.pdf</description>
<gates>
<gate name="G$1" symbol="DPC31"/>
<gate name="P" symbol="DPC31-P"/>
</gates>
<devices>
<device name="" package="QFP100R">
<connects>
<connect gate="G$1" pin="AGND" pad="7"/>
<connect gate="G$1" pin="ALE" pad="43"/>
<connect gate="G$1" pin="AVDD" pad="8"/>
<connect gate="G$1" pin="BOOT0" pad="81"/>
<connect gate="G$1" pin="BOOT1" pad="82"/>
<connect gate="G$1" pin="BUS0" pad="84"/>
<connect gate="G$1" pin="BUS1" pad="85"/>
<connect gate="G$1" pin="BUS2" pad="86"/>
<connect gate="G$1" pin="CLKOUTX2" pad="100"/>
<connect gate="G$1" pin="CLKOUTX4" pad="94"/>
<connect gate="G$1" pin="DBX" pad="83"/>
<connect gate="G$1" pin="NTEST1" pad="3"/>
<connect gate="G$1" pin="NTEST2" pad="4"/>
<connect gate="G$1" pin="PA0/AD0" pad="44"/>
<connect gate="G$1" pin="PA1/AD1" pad="45"/>
<connect gate="G$1" pin="PA2/AD2" pad="46"/>
<connect gate="G$1" pin="PA3/AD3" pad="47"/>
<connect gate="G$1" pin="PA4/AD4" pad="48"/>
<connect gate="G$1" pin="PA5/AD5" pad="49"/>
<connect gate="G$1" pin="PA6/AD6" pad="50"/>
<connect gate="G$1" pin="PA7/AD7" pad="51"/>
<connect gate="G$1" pin="PB0/P1.0/T2" pad="54"/>
<connect gate="G$1" pin="PB1/P1.1/T2EX" pad="55"/>
<connect gate="G$1" pin="PB2/P1.2/RES" pad="56"/>
<connect gate="G$1" pin="PB3/P1.3/IRR" pad="57"/>
<connect gate="G$1" pin="PB4/P1.4" pad="58"/>
<connect gate="G$1" pin="PB5/P1.5" pad="59"/>
<connect gate="G$1" pin="PB6/P1.6" pad="60"/>
<connect gate="G$1" pin="PB7/P1.7" pad="61"/>
<connect gate="G$1" pin="PC0/A8" pad="63"/>
<connect gate="G$1" pin="PC1/A9" pad="64"/>
<connect gate="G$1" pin="PC2/A10" pad="65"/>
<connect gate="G$1" pin="PC3/A11" pad="66"/>
<connect gate="G$1" pin="PC4/A12" pad="67"/>
<connect gate="G$1" pin="PC5/A13" pad="68"/>
<connect gate="G$1" pin="PC6/A14" pad="69"/>
<connect gate="G$1" pin="PC7/A15" pad="70"/>
<connect gate="G$1" pin="PD0/P3.0/RXD" pad="71"/>
<connect gate="G$1" pin="PD1/P3.1/TXD" pad="72"/>
<connect gate="G$1" pin="PD2/XINT0" pad="73"/>
<connect gate="G$1" pin="PD3/P3.3/XINT1" pad="74"/>
<connect gate="G$1" pin="PD4/P3.4/T0" pad="75"/>
<connect gate="G$1" pin="PD5/P3.5/T1" pad="76"/>
<connect gate="G$1" pin="PD6/XWR" pad="77"/>
<connect gate="G$1" pin="PD7/XRD" pad="78"/>
<connect gate="G$1" pin="PE0/D0" pad="10"/>
<connect gate="G$1" pin="PE1/D1" pad="11"/>
<connect gate="G$1" pin="PE2/D2" pad="12"/>
<connect gate="G$1" pin="PE3/D3" pad="13"/>
<connect gate="G$1" pin="PE4/D4" pad="14"/>
<connect gate="G$1" pin="PE5/D5" pad="15"/>
<connect gate="G$1" pin="PE6/D6" pad="16"/>
<connect gate="G$1" pin="PE7/D7" pad="17"/>
<connect gate="G$1" pin="PF0/A0" pad="18"/>
<connect gate="G$1" pin="PF1/A1" pad="19"/>
<connect gate="G$1" pin="PF2/A2" pad="20"/>
<connect gate="G$1" pin="PF3/A3" pad="21"/>
<connect gate="G$1" pin="PF4/A4" pad="22"/>
<connect gate="G$1" pin="PF5/A5" pad="23"/>
<connect gate="G$1" pin="PF6/A6" pad="24"/>
<connect gate="G$1" pin="PF7/A7" pad="25"/>
<connect gate="G$1" pin="PG0/A8" pad="26"/>
<connect gate="G$1" pin="PG1/A9" pad="27"/>
<connect gate="G$1" pin="PG2/A10" pad="30"/>
<connect gate="G$1" pin="PG3/A11" pad="31"/>
<connect gate="G$1" pin="PG4/A12" pad="32"/>
<connect gate="G$1" pin="PG5/XINT" pad="33"/>
<connect gate="G$1" pin="PG6/XCS" pad="34"/>
<connect gate="G$1" pin="PG7/XWR" pad="35"/>
<connect gate="G$1" pin="PH0/XRD" pad="36"/>
<connect gate="G$1" pin="PH1/VDD" pad="37"/>
<connect gate="G$1" pin="PH2/XRDY" pad="38"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="RTS_TXE" pad="96"/>
<connect gate="G$1" pin="RXD_RXS" pad="87"/>
<connect gate="G$1" pin="SSCLK" pad="92"/>
<connect gate="G$1" pin="SSDI" pad="90"/>
<connect gate="G$1" pin="SSDO" pad="93"/>
<connect gate="G$1" pin="TST1" pad="5"/>
<connect gate="G$1" pin="TXD_TXS" pad="95"/>
<connect gate="G$1" pin="XCSCODE" pad="41"/>
<connect gate="G$1" pin="XCSDATA" pad="39"/>
<connect gate="G$1" pin="XCTS_RXA" pad="88"/>
<connect gate="G$1" pin="XPLLEN" pad="89"/>
<connect gate="G$1" pin="XPSEN" pad="42"/>
<connect gate="G$1" pin="XTAL1" pad="98"/>
<connect gate="G$1" pin="XTAL2" pad="99"/>
<connect gate="P" pin="GND" pad="1"/>
<connect gate="P" pin="GND@1" pad="9"/>
<connect gate="P" pin="GND@2" pad="28"/>
<connect gate="P" pin="GND@3" pad="40"/>
<connect gate="P" pin="GND@4" pad="53"/>
<connect gate="P" pin="GND@5" pad="62"/>
<connect gate="P" pin="GND@6" pad="80"/>
<connect gate="P" pin="GND@7" pad="91"/>
<connect gate="P" pin="GND@8" pad="97"/>
<connect gate="P" pin="VCC" pad="2"/>
<connect gate="P" pin="VCC@1" pad="29"/>
<connect gate="P" pin="VCC@2" pad="52"/>
<connect gate="P" pin="VCC@3" pad="79"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="8*C535" prefix="IC">
<description>&lt;b&gt;80C515/80C535  8-Bit CMOS Single-Chip Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/cmc_upload/migrated_files/document_files/Datasheet/d80515.pdf&lt;br&gt;
&lt;b&gt;This device has been discontinued !!!&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="80C535-1"/>
<gate name="P" symbol="2VCC1GND"/>
</gates>
<devices>
<device name="M" package="MQFP80-1">
<connects>
<connect gate="G$1" pin="ALE" pad="48"/>
<connect gate="G$1" pin="CLKOUTP1.6" pad="25"/>
<connect gate="G$1" pin="EA" pad="49"/>
<connect gate="G$1" pin="INT2/P1.4" pad="27"/>
<connect gate="G$1" pin="INT3/P1.0" pad="31"/>
<connect gate="G$1" pin="INT4/P1.1" pad="30"/>
<connect gate="G$1" pin="INT5/P1.2" pad="29"/>
<connect gate="G$1" pin="INT6/P1.3" pad="28"/>
<connect gate="G$1" pin="P0.0" pad="52"/>
<connect gate="G$1" pin="P0.1" pad="53"/>
<connect gate="G$1" pin="P0.2" pad="54"/>
<connect gate="G$1" pin="P0.3" pad="55"/>
<connect gate="G$1" pin="P0.4" pad="56"/>
<connect gate="G$1" pin="P0.5" pad="57"/>
<connect gate="G$1" pin="P0.6" pad="58"/>
<connect gate="G$1" pin="P0.7" pad="59"/>
<connect gate="G$1" pin="P2.0" pad="38"/>
<connect gate="G$1" pin="P2.1" pad="39"/>
<connect gate="G$1" pin="P2.2" pad="40"/>
<connect gate="G$1" pin="P2.3" pad="41"/>
<connect gate="G$1" pin="P2.4" pad="42"/>
<connect gate="G$1" pin="P2.5" pad="43"/>
<connect gate="G$1" pin="P2.6" pad="44"/>
<connect gate="G$1" pin="P2.7" pad="45"/>
<connect gate="G$1" pin="P3.0" pad="15"/>
<connect gate="G$1" pin="P3.1" pad="16"/>
<connect gate="G$1" pin="P3.2" pad="17"/>
<connect gate="G$1" pin="P3.3" pad="18"/>
<connect gate="G$1" pin="P3.4/T0" pad="19"/>
<connect gate="G$1" pin="P3.5/T1" pad="20"/>
<connect gate="G$1" pin="P3.6/WR" pad="21"/>
<connect gate="G$1" pin="P3.7/RD" pad="22"/>
<connect gate="G$1" pin="P4.0" pad="72"/>
<connect gate="G$1" pin="P4.1" pad="73"/>
<connect gate="G$1" pin="P4.2" pad="74"/>
<connect gate="G$1" pin="P4.3" pad="76"/>
<connect gate="G$1" pin="P4.4" pad="77"/>
<connect gate="G$1" pin="P4.5" pad="78"/>
<connect gate="G$1" pin="P4.6" pad="79"/>
<connect gate="G$1" pin="P4.7" pad="80"/>
<connect gate="G$1" pin="P5.0" pad="67"/>
<connect gate="G$1" pin="P5.1" pad="66"/>
<connect gate="G$1" pin="P5.2" pad="65"/>
<connect gate="G$1" pin="P5.3" pad="64"/>
<connect gate="G$1" pin="P5.4" pad="63"/>
<connect gate="G$1" pin="P5.5" pad="62"/>
<connect gate="G$1" pin="P5.6" pad="61"/>
<connect gate="G$1" pin="P5.7" pad="60"/>
<connect gate="G$1" pin="P6.0" pad="12"/>
<connect gate="G$1" pin="P6.1" pad="11"/>
<connect gate="G$1" pin="P6.2" pad="10"/>
<connect gate="G$1" pin="P6.3" pad="9"/>
<connect gate="G$1" pin="P6.4" pad="8"/>
<connect gate="G$1" pin="P6.5" pad="7"/>
<connect gate="G$1" pin="P6.6" pad="6"/>
<connect gate="G$1" pin="P6.7" pad="5"/>
<connect gate="G$1" pin="PE" pad="75"/>
<connect gate="G$1" pin="PSEN" pad="47"/>
<connect gate="G$1" pin="RESET" pad="1"/>
<connect gate="G$1" pin="T2/P1.7" pad="24"/>
<connect gate="G$1" pin="T2EX/P1.5" pad="26"/>
<connect gate="G$1" pin="VAGND" pad="4"/>
<connect gate="G$1" pin="VAREF" pad="3"/>
<connect gate="G$1" pin="XTAL1" pad="37"/>
<connect gate="G$1" pin="XTAL2" pad="36"/>
<connect gate="P" pin="GND@1" pad="34"/>
<connect gate="P" pin="VCC@1" pad="33"/>
<connect gate="P" pin="VCC@2" pad="69"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N" package="PLCC68">
<connects>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="CLKOUTP1.6" pad="30"/>
<connect gate="G$1" pin="EA" pad="51"/>
<connect gate="G$1" pin="INT2/P1.4" pad="32"/>
<connect gate="G$1" pin="INT3/P1.0" pad="36"/>
<connect gate="G$1" pin="INT4/P1.1" pad="35"/>
<connect gate="G$1" pin="INT5/P1.2" pad="34"/>
<connect gate="G$1" pin="INT6/P1.3" pad="33"/>
<connect gate="G$1" pin="P0.0" pad="52"/>
<connect gate="G$1" pin="P0.1" pad="53"/>
<connect gate="G$1" pin="P0.2" pad="54"/>
<connect gate="G$1" pin="P0.3" pad="55"/>
<connect gate="G$1" pin="P0.4" pad="56"/>
<connect gate="G$1" pin="P0.5" pad="57"/>
<connect gate="G$1" pin="P0.6" pad="58"/>
<connect gate="G$1" pin="P0.7" pad="59"/>
<connect gate="G$1" pin="P2.0" pad="41"/>
<connect gate="G$1" pin="P2.1" pad="42"/>
<connect gate="G$1" pin="P2.2" pad="43"/>
<connect gate="G$1" pin="P2.3" pad="44"/>
<connect gate="G$1" pin="P2.4" pad="45"/>
<connect gate="G$1" pin="P2.5" pad="46"/>
<connect gate="G$1" pin="P2.6" pad="47"/>
<connect gate="G$1" pin="P2.7" pad="48"/>
<connect gate="G$1" pin="P3.0" pad="21"/>
<connect gate="G$1" pin="P3.1" pad="22"/>
<connect gate="G$1" pin="P3.2" pad="23"/>
<connect gate="G$1" pin="P3.3" pad="24"/>
<connect gate="G$1" pin="P3.4/T0" pad="25"/>
<connect gate="G$1" pin="P3.5/T1" pad="26"/>
<connect gate="G$1" pin="P3.6/WR" pad="27"/>
<connect gate="G$1" pin="P3.7/RD" pad="28"/>
<connect gate="G$1" pin="P4.0" pad="1"/>
<connect gate="G$1" pin="P4.1" pad="2"/>
<connect gate="G$1" pin="P4.2" pad="3"/>
<connect gate="G$1" pin="P4.3" pad="5"/>
<connect gate="G$1" pin="P4.4" pad="6"/>
<connect gate="G$1" pin="P4.5" pad="7"/>
<connect gate="G$1" pin="P4.6" pad="8"/>
<connect gate="G$1" pin="P4.7" pad="9"/>
<connect gate="G$1" pin="P5.0" pad="67"/>
<connect gate="G$1" pin="P5.1" pad="66"/>
<connect gate="G$1" pin="P5.2" pad="65"/>
<connect gate="G$1" pin="P5.3" pad="64"/>
<connect gate="G$1" pin="P5.4" pad="63"/>
<connect gate="G$1" pin="P5.5" pad="62"/>
<connect gate="G$1" pin="P5.6" pad="61"/>
<connect gate="G$1" pin="P5.7" pad="60"/>
<connect gate="G$1" pin="P6.0" pad="20"/>
<connect gate="G$1" pin="P6.1" pad="19"/>
<connect gate="G$1" pin="P6.2" pad="18"/>
<connect gate="G$1" pin="P6.3" pad="17"/>
<connect gate="G$1" pin="P6.4" pad="16"/>
<connect gate="G$1" pin="P6.5" pad="15"/>
<connect gate="G$1" pin="P6.6" pad="14"/>
<connect gate="G$1" pin="P6.7" pad="13"/>
<connect gate="G$1" pin="PE" pad="4"/>
<connect gate="G$1" pin="PSEN" pad="49"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="T2/P1.7" pad="29"/>
<connect gate="G$1" pin="T2EX/P1.5" pad="31"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="GND@1" pad="38"/>
<connect gate="P" pin="VCC@1" pad="37"/>
<connect gate="P" pin="VCC@2" pad="68"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N-S" package="PLCC68SOCK">
<connects>
<connect gate="G$1" pin="ALE" pad="50"/>
<connect gate="G$1" pin="CLKOUTP1.6" pad="30"/>
<connect gate="G$1" pin="EA" pad="51"/>
<connect gate="G$1" pin="INT2/P1.4" pad="32"/>
<connect gate="G$1" pin="INT3/P1.0" pad="36"/>
<connect gate="G$1" pin="INT4/P1.1" pad="35"/>
<connect gate="G$1" pin="INT5/P1.2" pad="34"/>
<connect gate="G$1" pin="INT6/P1.3" pad="33"/>
<connect gate="G$1" pin="P0.0" pad="52"/>
<connect gate="G$1" pin="P0.1" pad="53"/>
<connect gate="G$1" pin="P0.2" pad="54"/>
<connect gate="G$1" pin="P0.3" pad="55"/>
<connect gate="G$1" pin="P0.4" pad="56"/>
<connect gate="G$1" pin="P0.5" pad="57"/>
<connect gate="G$1" pin="P0.6" pad="58"/>
<connect gate="G$1" pin="P0.7" pad="59"/>
<connect gate="G$1" pin="P2.0" pad="41"/>
<connect gate="G$1" pin="P2.1" pad="42"/>
<connect gate="G$1" pin="P2.2" pad="43"/>
<connect gate="G$1" pin="P2.3" pad="44"/>
<connect gate="G$1" pin="P2.4" pad="45"/>
<connect gate="G$1" pin="P2.5" pad="46"/>
<connect gate="G$1" pin="P2.6" pad="47"/>
<connect gate="G$1" pin="P2.7" pad="48"/>
<connect gate="G$1" pin="P3.0" pad="21"/>
<connect gate="G$1" pin="P3.1" pad="22"/>
<connect gate="G$1" pin="P3.2" pad="23"/>
<connect gate="G$1" pin="P3.3" pad="24"/>
<connect gate="G$1" pin="P3.4/T0" pad="25"/>
<connect gate="G$1" pin="P3.5/T1" pad="26"/>
<connect gate="G$1" pin="P3.6/WR" pad="27"/>
<connect gate="G$1" pin="P3.7/RD" pad="28"/>
<connect gate="G$1" pin="P4.0" pad="1"/>
<connect gate="G$1" pin="P4.1" pad="2"/>
<connect gate="G$1" pin="P4.2" pad="3"/>
<connect gate="G$1" pin="P4.3" pad="5"/>
<connect gate="G$1" pin="P4.4" pad="6"/>
<connect gate="G$1" pin="P4.5" pad="7"/>
<connect gate="G$1" pin="P4.6" pad="8"/>
<connect gate="G$1" pin="P4.7" pad="9"/>
<connect gate="G$1" pin="P5.0" pad="67"/>
<connect gate="G$1" pin="P5.1" pad="66"/>
<connect gate="G$1" pin="P5.2" pad="65"/>
<connect gate="G$1" pin="P5.3" pad="64"/>
<connect gate="G$1" pin="P5.4" pad="63"/>
<connect gate="G$1" pin="P5.5" pad="62"/>
<connect gate="G$1" pin="P5.6" pad="61"/>
<connect gate="G$1" pin="P5.7" pad="60"/>
<connect gate="G$1" pin="P6.0" pad="20"/>
<connect gate="G$1" pin="P6.1" pad="19"/>
<connect gate="G$1" pin="P6.2" pad="18"/>
<connect gate="G$1" pin="P6.3" pad="17"/>
<connect gate="G$1" pin="P6.4" pad="16"/>
<connect gate="G$1" pin="P6.5" pad="15"/>
<connect gate="G$1" pin="P6.6" pad="14"/>
<connect gate="G$1" pin="P6.7" pad="13"/>
<connect gate="G$1" pin="PE" pad="4"/>
<connect gate="G$1" pin="PSEN" pad="49"/>
<connect gate="G$1" pin="RESET" pad="10"/>
<connect gate="G$1" pin="T2/P1.7" pad="29"/>
<connect gate="G$1" pin="T2EX/P1.5" pad="31"/>
<connect gate="G$1" pin="VAGND" pad="12"/>
<connect gate="G$1" pin="VAREF" pad="11"/>
<connect gate="G$1" pin="XTAL1" pad="40"/>
<connect gate="G$1" pin="XTAL2" pad="39"/>
<connect gate="P" pin="GND@1" pad="38"/>
<connect gate="P" pin="VCC@1" pad="37"/>
<connect gate="P" pin="VCC@2" pad="68"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTS428L2" prefix="IC">
<description>&lt;b&gt;Smart High-Side Power Switch&lt;/b&gt;&lt;p&gt;
One Channel: 60mOhm Status Feedback&lt;br&gt;
Source: Source: www.infineon.com .. BTS428L2_20030912.pdf</description>
<gates>
<gate name="G$1" symbol="BTS428L2"/>
</gates>
<devices>
<device name="" package="TO252-5-11">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="ST" pad="4"/>
<connect gate="G$1" pin="VBB" pad="TAB"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BTS555" prefix="IC">
<description>&lt;b&gt;Smart Highside High Current Power Switch&lt;/b&gt; PROFET®&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com/upload/Document/cmc_upload/documents/011/8726/Datasheet_BTS555.pdf</description>
<gates>
<gate name="G$1" symbol="BTS555"/>
</gates>
<devices>
<device name="" package="TO220-51">
<connects>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="IS" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="VBB" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="BTS555."/>
<attribute name="OC_FARNELL" value="4109260"/>
<attribute name="OC_NEWARK" value="26H6766"/>
</technology>
</technologies>
</device>
<device name="E3146" package="TO220-52">
<connects>
<connect gate="G$1" pin="IN" pad="2"/>
<connect gate="G$1" pin="IS" pad="4"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="5"/>
<connect gate="G$1" pin="VBB" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA*-C161CS" prefix="IC" uservalue="yes">
<description>16bit  Low-Cost Microcontroller mit CAN</description>
<gates>
<gate name="G" symbol="SABC161CS"/>
<gate name="G$1" symbol="PWR"/>
<gate name="G$2" symbol="PWR"/>
<gate name="G$3" symbol="PWR"/>
<gate name="G$4" symbol="PWR"/>
<gate name="G$5" symbol="PWR"/>
<gate name="G$6" symbol="PWR"/>
<gate name="G$7" symbol="PWR"/>
<gate name="G$8" symbol="PWR"/>
<gate name="G$9" symbol="PWR"/>
<gate name="G$10" symbol="PWR"/>
<gate name="G$11" symbol="APWR"/>
<gate name="G$13" symbol="VSS-1"/>
</gates>
<devices>
<device name="SMD" package="P-TQFP-128">
<connects>
<connect gate="G" pin="!NMI" pad="2"/>
<connect gate="G" pin="ALE" pad="83"/>
<connect gate="G" pin="BHE/WRH/P3.12" pad="65"/>
<connect gate="G" pin="CANRXD0/P4.4/A20" pad="74"/>
<connect gate="G" pin="CANRXD1/P4.3/A19" pad="73"/>
<connect gate="G" pin="CANTXD0/P4.6/A22" pad="76"/>
<connect gate="G" pin="CANTXD1/P4.5/A21" pad="75"/>
<connect gate="G" pin="CAPIN/P3.2" pad="55"/>
<connect gate="G" pin="CC24IO/P1H.4/A12" pad="117"/>
<connect gate="G" pin="CC25IO/P1H.5/A13" pad="118"/>
<connect gate="G" pin="CC26IO/P1H.6/A14" pad="119"/>
<connect gate="G" pin="CC27IO/P1H.7/A15" pad="120"/>
<connect gate="G" pin="EA" pad="84"/>
<connect gate="G" pin="FOUT/CLKOUT/P3.15" pad="67"/>
<connect gate="G" pin="MRST/P3.8" pad="61"/>
<connect gate="G" pin="MTSR/P3.9" pad="62"/>
<connect gate="G" pin="P0H.0/AD8" pad="95"/>
<connect gate="G" pin="P0H.1/AD9" pad="96"/>
<connect gate="G" pin="P0H.2/AD10" pad="97"/>
<connect gate="G" pin="P0H.3/AD11" pad="98"/>
<connect gate="G" pin="P0H.4/AD12" pad="99"/>
<connect gate="G" pin="P0H.5/AD13" pad="100"/>
<connect gate="G" pin="P0H.6/AD14" pad="101"/>
<connect gate="G" pin="P0H.7/AD15" pad="102"/>
<connect gate="G" pin="P0L.0/AD0" pad="85"/>
<connect gate="G" pin="P0L.1/AD1" pad="86"/>
<connect gate="G" pin="P0L.2/AD2" pad="87"/>
<connect gate="G" pin="P0L.3/AD3" pad="88"/>
<connect gate="G" pin="P0L.4/AD4" pad="89"/>
<connect gate="G" pin="P0L.5/AD5" pad="90"/>
<connect gate="G" pin="P0L.6/AD6" pad="91"/>
<connect gate="G" pin="P0L.7/AD7" pad="92"/>
<connect gate="G" pin="P1H.0/A8" pad="113"/>
<connect gate="G" pin="P1H.1/A9" pad="114"/>
<connect gate="G" pin="P1H.2/A10" pad="115"/>
<connect gate="G" pin="P1H.3/A11" pad="116"/>
<connect gate="G" pin="P1L.0/A0" pad="103"/>
<connect gate="G" pin="P1L.1/A1" pad="104"/>
<connect gate="G" pin="P1L.2/A2" pad="105"/>
<connect gate="G" pin="P1L.3/A3" pad="106"/>
<connect gate="G" pin="P1L.4/A4" pad="107"/>
<connect gate="G" pin="P1L.5/A5" pad="108"/>
<connect gate="G" pin="P1L.6/A6" pad="109"/>
<connect gate="G" pin="P1L.7/A7" pad="110"/>
<connect gate="G" pin="P2.10" pad="45"/>
<connect gate="G" pin="P2.11" pad="46"/>
<connect gate="G" pin="P2.12" pad="47"/>
<connect gate="G" pin="P2.13" pad="48"/>
<connect gate="G" pin="P2.14" pad="49"/>
<connect gate="G" pin="P2.15" pad="50"/>
<connect gate="G" pin="P2.8" pad="43"/>
<connect gate="G" pin="P2.9" pad="44"/>
<connect gate="G" pin="P4.0/A16" pad="70"/>
<connect gate="G" pin="P4.1/A17" pad="71"/>
<connect gate="G" pin="P4.2/A18" pad="72"/>
<connect gate="G" pin="P4.7/A23" pad="77"/>
<connect gate="G" pin="P5.0/AN0" pad="27"/>
<connect gate="G" pin="P5.1/AN1" pad="28"/>
<connect gate="G" pin="P5.12" pad="37"/>
<connect gate="G" pin="P5.13" pad="38"/>
<connect gate="G" pin="P5.14" pad="39"/>
<connect gate="G" pin="P5.15" pad="40"/>
<connect gate="G" pin="P5.2/AN2" pad="29"/>
<connect gate="G" pin="P5.3/AN3" pad="30"/>
<connect gate="G" pin="P5.4/AN4" pad="31"/>
<connect gate="G" pin="P5.5/AN5" pad="32"/>
<connect gate="G" pin="P5.6/AN6" pad="33"/>
<connect gate="G" pin="P5.7/AN7" pad="34"/>
<connect gate="G" pin="P6.0/CS0" pad="5"/>
<connect gate="G" pin="P6.1/CS1" pad="6"/>
<connect gate="G" pin="P6.2/CS2" pad="7"/>
<connect gate="G" pin="P6.3/CS3" pad="8"/>
<connect gate="G" pin="P6.4/CS4" pad="9"/>
<connect gate="G" pin="P6.5/HOLD" pad="10"/>
<connect gate="G" pin="P6.6/HLDA" pad="11"/>
<connect gate="G" pin="P6.7/BREQ" pad="12"/>
<connect gate="G" pin="P7.4/CC28IO" pad="13"/>
<connect gate="G" pin="P7.5/CC29IO" pad="14"/>
<connect gate="G" pin="P7.6/CC30IO" pad="15"/>
<connect gate="G" pin="P7.7/CC31IO" pad="16"/>
<connect gate="G" pin="P9.0/SDA0" pad="19"/>
<connect gate="G" pin="P9.1/SCL0" pad="20"/>
<connect gate="G" pin="P9.2/SDA1" pad="21"/>
<connect gate="G" pin="P9.3/SCL1" pad="22"/>
<connect gate="G" pin="P9.4/SDA2" pad="23"/>
<connect gate="G" pin="P9.5" pad="24"/>
<connect gate="G" pin="RD" pad="80"/>
<connect gate="G" pin="READY" pad="82"/>
<connect gate="G" pin="RSTIN" pad="128"/>
<connect gate="G" pin="RSTOUT" pad="1"/>
<connect gate="G" pin="RXD0/P3.11" pad="64"/>
<connect gate="G" pin="RXD1/T6OUT/P3.1" pad="54"/>
<connect gate="G" pin="SCLK/P3.13" pad="66"/>
<connect gate="G" pin="T2IN/P3.7" pad="60"/>
<connect gate="G" pin="T3EUD/P3.4" pad="57"/>
<connect gate="G" pin="T3IN/P3.6" pad="59"/>
<connect gate="G" pin="T3OUT/P3.3" pad="56"/>
<connect gate="G" pin="T4IN/P3.5" pad="58"/>
<connect gate="G" pin="TXD0/P3.10" pad="63"/>
<connect gate="G" pin="TXD1/T0IN/P3.0" pad="53"/>
<connect gate="G" pin="WR/WRL" pad="81"/>
<connect gate="G" pin="XTAL1" pad="124"/>
<connect gate="G" pin="XTAL2" pad="123"/>
<connect gate="G" pin="XTAL3" pad="126"/>
<connect gate="G" pin="XTAL4" pad="127"/>
<connect gate="G$1" pin="VDD@0" pad="121"/>
<connect gate="G$1" pin="VSS@0" pad="122"/>
<connect gate="G$10" pin="VDD@0" pad="68"/>
<connect gate="G$10" pin="VSS@0" pad="69"/>
<connect gate="G$11" pin="VAGND" pad="36"/>
<connect gate="G$11" pin="VAREF" pad="35"/>
<connect gate="G$13" pin="VSS" pad="125"/>
<connect gate="G$2" pin="VDD@0" pad="4"/>
<connect gate="G$2" pin="VSS@0" pad="3"/>
<connect gate="G$3" pin="VDD@0" pad="18"/>
<connect gate="G$3" pin="VSS@0" pad="17"/>
<connect gate="G$4" pin="VDD@0" pad="26"/>
<connect gate="G$4" pin="VSS@0" pad="25"/>
<connect gate="G$5" pin="VDD@0" pad="42"/>
<connect gate="G$5" pin="VSS@0" pad="41"/>
<connect gate="G$6" pin="VDD@0" pad="52"/>
<connect gate="G$6" pin="VSS@0" pad="51"/>
<connect gate="G$7" pin="VDD@0" pad="93"/>
<connect gate="G$7" pin="VSS@0" pad="94"/>
<connect gate="G$8" pin="VDD@0" pad="111"/>
<connect gate="G$8" pin="VSS@0" pad="112"/>
<connect gate="G$9" pin="VDD@0" pad="78"/>
<connect gate="G$9" pin="VSS@0" pad="79"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1472739"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA*-C165-RF" prefix="IC">
<description>&lt;b&gt;16 bit MICROPROCESSOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C165-1"/>
<gate name="P" symbol="6_VCCVSS"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G$1" pin="!EA" pad="37"/>
<connect gate="G$1" pin="!NMI" pad="81"/>
<connect gate="G$1" pin="!RD" pad="33"/>
<connect gate="G$1" pin="!READY" pad="35"/>
<connect gate="G$1" pin="!RSTIN" pad="79"/>
<connect gate="G$1" pin="!RSTOUT" pad="80"/>
<connect gate="G$1" pin="!WR!/!WRL" pad="34"/>
<connect gate="G$1" pin="ALE" pad="36"/>
<connect gate="G$1" pin="P0H-0" pad="51"/>
<connect gate="G$1" pin="P0H-1" pad="52"/>
<connect gate="G$1" pin="P0H-2" pad="53"/>
<connect gate="G$1" pin="P0H-3" pad="54"/>
<connect gate="G$1" pin="P0H-4" pad="55"/>
<connect gate="G$1" pin="P0H-5" pad="56"/>
<connect gate="G$1" pin="P0H-6" pad="57"/>
<connect gate="G$1" pin="P0H-7" pad="58"/>
<connect gate="G$1" pin="P0L-0" pad="41"/>
<connect gate="G$1" pin="P0L-1" pad="42"/>
<connect gate="G$1" pin="P0L-2" pad="43"/>
<connect gate="G$1" pin="P0L-3" pad="44"/>
<connect gate="G$1" pin="P0L-4" pad="45"/>
<connect gate="G$1" pin="P0L-5" pad="46"/>
<connect gate="G$1" pin="P0L-6" pad="47"/>
<connect gate="G$1" pin="P0L-7" pad="48"/>
<connect gate="G$1" pin="P1H-0" pad="67"/>
<connect gate="G$1" pin="P1H-1" pad="68"/>
<connect gate="G$1" pin="P1H-2" pad="71"/>
<connect gate="G$1" pin="P1H-3" pad="72"/>
<connect gate="G$1" pin="P1H-4" pad="73"/>
<connect gate="G$1" pin="P1H-5" pad="74"/>
<connect gate="G$1" pin="P1H-6" pad="75"/>
<connect gate="G$1" pin="P1H-7" pad="76"/>
<connect gate="G$1" pin="P1L-0" pad="59"/>
<connect gate="G$1" pin="P1L-1" pad="60"/>
<connect gate="G$1" pin="P1L-2" pad="61"/>
<connect gate="G$1" pin="P1L-3" pad="62"/>
<connect gate="G$1" pin="P1L-4" pad="63"/>
<connect gate="G$1" pin="P1L-5" pad="64"/>
<connect gate="G$1" pin="P1L-6" pad="65"/>
<connect gate="G$1" pin="P1L-7" pad="66"/>
<connect gate="G$1" pin="P2-10" pad="92"/>
<connect gate="G$1" pin="P2-11" pad="93"/>
<connect gate="G$1" pin="P2-12" pad="94"/>
<connect gate="G$1" pin="P2-13" pad="95"/>
<connect gate="G$1" pin="P2-14" pad="96"/>
<connect gate="G$1" pin="P2-15" pad="97"/>
<connect gate="G$1" pin="P2-8" pad="90"/>
<connect gate="G$1" pin="P2-9" pad="91"/>
<connect gate="G$1" pin="P3-0" pad="8"/>
<connect gate="G$1" pin="P3-1" pad="9"/>
<connect gate="G$1" pin="P3-10" pad="18"/>
<connect gate="G$1" pin="P3-11" pad="19"/>
<connect gate="G$1" pin="P3-12" pad="20"/>
<connect gate="G$1" pin="P3-13" pad="21"/>
<connect gate="G$1" pin="P3-15" pad="22"/>
<connect gate="G$1" pin="P3-2" pad="10"/>
<connect gate="G$1" pin="P3-3" pad="11"/>
<connect gate="G$1" pin="P3-4" pad="12"/>
<connect gate="G$1" pin="P3-5" pad="13"/>
<connect gate="G$1" pin="P3-6" pad="14"/>
<connect gate="G$1" pin="P3-7" pad="15"/>
<connect gate="G$1" pin="P3-8" pad="16"/>
<connect gate="G$1" pin="P3-9" pad="17"/>
<connect gate="G$1" pin="P4-0" pad="23"/>
<connect gate="G$1" pin="P4-1" pad="24"/>
<connect gate="G$1" pin="P4-2" pad="25"/>
<connect gate="G$1" pin="P4-3" pad="26"/>
<connect gate="G$1" pin="P4-4" pad="29"/>
<connect gate="G$1" pin="P4-5" pad="30"/>
<connect gate="G$1" pin="P4-6" pad="31"/>
<connect gate="G$1" pin="P4-7" pad="32"/>
<connect gate="G$1" pin="P5-10" pad="98"/>
<connect gate="G$1" pin="P5-11" pad="99"/>
<connect gate="G$1" pin="P5-12" pad="100"/>
<connect gate="G$1" pin="P5-13" pad="1"/>
<connect gate="G$1" pin="P5-14" pad="2"/>
<connect gate="G$1" pin="P5-15" pad="3"/>
<connect gate="G$1" pin="P6-0" pad="82"/>
<connect gate="G$1" pin="P6-1" pad="83"/>
<connect gate="G$1" pin="P6-2" pad="84"/>
<connect gate="G$1" pin="P6-3" pad="85"/>
<connect gate="G$1" pin="P6-4" pad="86"/>
<connect gate="G$1" pin="P6-5" pad="87"/>
<connect gate="G$1" pin="P6-6" pad="88"/>
<connect gate="G$1" pin="P6-7" pad="89"/>
<connect gate="G$1" pin="VPP" pad="40"/>
<connect gate="G$1" pin="XTAL1" pad="5"/>
<connect gate="G$1" pin="XTAL2" pad="6"/>
<connect gate="P" pin="VCC@1" pad="7"/>
<connect gate="P" pin="VCC@2" pad="28"/>
<connect gate="P" pin="VCC@3" pad="38"/>
<connect gate="P" pin="VCC@4" pad="49"/>
<connect gate="P" pin="VCC@5" pad="69"/>
<connect gate="P" pin="VCC@6" pad="78"/>
<connect gate="P" pin="VSS@1" pad="4"/>
<connect gate="P" pin="VSS@2" pad="27"/>
<connect gate="P" pin="VSS@3" pad="39"/>
<connect gate="P" pin="VSS@4" pad="50"/>
<connect gate="P" pin="VSS@5" pad="70"/>
<connect gate="P" pin="VSS@6" pad="77"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA*-C165-RM" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C165-1"/>
<gate name="P" symbol="6_VCCVSS"/>
</gates>
<devices>
<device name="" package="MQFP100">
<connects>
<connect gate="G$1" pin="!EA" pad="39"/>
<connect gate="G$1" pin="!NMI" pad="83"/>
<connect gate="G$1" pin="!RD" pad="35"/>
<connect gate="G$1" pin="!READY" pad="37"/>
<connect gate="G$1" pin="!RSTIN" pad="81"/>
<connect gate="G$1" pin="!RSTOUT" pad="82"/>
<connect gate="G$1" pin="!WR!/!WRL" pad="36"/>
<connect gate="G$1" pin="ALE" pad="38"/>
<connect gate="G$1" pin="P0H-0" pad="53"/>
<connect gate="G$1" pin="P0H-1" pad="54"/>
<connect gate="G$1" pin="P0H-2" pad="55"/>
<connect gate="G$1" pin="P0H-3" pad="56"/>
<connect gate="G$1" pin="P0H-4" pad="57"/>
<connect gate="G$1" pin="P0H-5" pad="58"/>
<connect gate="G$1" pin="P0H-6" pad="59"/>
<connect gate="G$1" pin="P0H-7" pad="60"/>
<connect gate="G$1" pin="P0L-0" pad="43"/>
<connect gate="G$1" pin="P0L-1" pad="44"/>
<connect gate="G$1" pin="P0L-2" pad="45"/>
<connect gate="G$1" pin="P0L-3" pad="46"/>
<connect gate="G$1" pin="P0L-4" pad="47"/>
<connect gate="G$1" pin="P0L-5" pad="48"/>
<connect gate="G$1" pin="P0L-6" pad="49"/>
<connect gate="G$1" pin="P0L-7" pad="50"/>
<connect gate="G$1" pin="P1H-0" pad="69"/>
<connect gate="G$1" pin="P1H-1" pad="70"/>
<connect gate="G$1" pin="P1H-2" pad="73"/>
<connect gate="G$1" pin="P1H-3" pad="74"/>
<connect gate="G$1" pin="P1H-4" pad="75"/>
<connect gate="G$1" pin="P1H-5" pad="76"/>
<connect gate="G$1" pin="P1H-6" pad="77"/>
<connect gate="G$1" pin="P1H-7" pad="78"/>
<connect gate="G$1" pin="P1L-0" pad="61"/>
<connect gate="G$1" pin="P1L-1" pad="62"/>
<connect gate="G$1" pin="P1L-2" pad="63"/>
<connect gate="G$1" pin="P1L-3" pad="64"/>
<connect gate="G$1" pin="P1L-4" pad="65"/>
<connect gate="G$1" pin="P1L-5" pad="66"/>
<connect gate="G$1" pin="P1L-6" pad="67"/>
<connect gate="G$1" pin="P1L-7" pad="68"/>
<connect gate="G$1" pin="P2-10" pad="94"/>
<connect gate="G$1" pin="P2-11" pad="95"/>
<connect gate="G$1" pin="P2-12" pad="96"/>
<connect gate="G$1" pin="P2-13" pad="97"/>
<connect gate="G$1" pin="P2-14" pad="98"/>
<connect gate="G$1" pin="P2-15" pad="99"/>
<connect gate="G$1" pin="P2-8" pad="92"/>
<connect gate="G$1" pin="P2-9" pad="93"/>
<connect gate="G$1" pin="P3-0" pad="10"/>
<connect gate="G$1" pin="P3-1" pad="11"/>
<connect gate="G$1" pin="P3-10" pad="20"/>
<connect gate="G$1" pin="P3-11" pad="21"/>
<connect gate="G$1" pin="P3-12" pad="22"/>
<connect gate="G$1" pin="P3-13" pad="23"/>
<connect gate="G$1" pin="P3-15" pad="24"/>
<connect gate="G$1" pin="P3-2" pad="12"/>
<connect gate="G$1" pin="P3-3" pad="13"/>
<connect gate="G$1" pin="P3-4" pad="14"/>
<connect gate="G$1" pin="P3-5" pad="15"/>
<connect gate="G$1" pin="P3-6" pad="16"/>
<connect gate="G$1" pin="P3-7" pad="17"/>
<connect gate="G$1" pin="P3-8" pad="18"/>
<connect gate="G$1" pin="P3-9" pad="19"/>
<connect gate="G$1" pin="P4-0" pad="25"/>
<connect gate="G$1" pin="P4-1" pad="26"/>
<connect gate="G$1" pin="P4-2" pad="27"/>
<connect gate="G$1" pin="P4-3" pad="28"/>
<connect gate="G$1" pin="P4-4" pad="31"/>
<connect gate="G$1" pin="P4-5" pad="32"/>
<connect gate="G$1" pin="P4-6" pad="33"/>
<connect gate="G$1" pin="P4-7" pad="34"/>
<connect gate="G$1" pin="P5-10" pad="100"/>
<connect gate="G$1" pin="P5-11" pad="1"/>
<connect gate="G$1" pin="P5-12" pad="2"/>
<connect gate="G$1" pin="P5-13" pad="3"/>
<connect gate="G$1" pin="P5-14" pad="4"/>
<connect gate="G$1" pin="P5-15" pad="5"/>
<connect gate="G$1" pin="P6-0" pad="84"/>
<connect gate="G$1" pin="P6-1" pad="85"/>
<connect gate="G$1" pin="P6-2" pad="86"/>
<connect gate="G$1" pin="P6-3" pad="87"/>
<connect gate="G$1" pin="P6-4" pad="88"/>
<connect gate="G$1" pin="P6-5" pad="89"/>
<connect gate="G$1" pin="P6-6" pad="90"/>
<connect gate="G$1" pin="P6-7" pad="91"/>
<connect gate="G$1" pin="VPP" pad="42"/>
<connect gate="G$1" pin="XTAL1" pad="7"/>
<connect gate="G$1" pin="XTAL2" pad="8"/>
<connect gate="P" pin="VCC@1" pad="9"/>
<connect gate="P" pin="VCC@2" pad="30"/>
<connect gate="P" pin="VCC@3" pad="40"/>
<connect gate="P" pin="VCC@4" pad="51"/>
<connect gate="P" pin="VCC@5" pad="71"/>
<connect gate="P" pin="VCC@6" pad="80"/>
<connect gate="P" pin="VSS@1" pad="6"/>
<connect gate="P" pin="VSS@2" pad="29"/>
<connect gate="P" pin="VSS@3" pad="41"/>
<connect gate="P" pin="VSS@4" pad="52"/>
<connect gate="P" pin="VSS@5" pad="72"/>
<connect gate="P" pin="VSS@6" pad="79"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA*-C167-LM" prefix="IC">
<description>&lt;b&gt;MICROPROCESSOR/PERIPHERAL DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="C167-1"/>
<gate name="P" symbol="10VCCVSS"/>
</gates>
<devices>
<device name="" package="MQFP144-RND">
<connects>
<connect gate="G$1" pin="!EA" pad="99"/>
<connect gate="G$1" pin="!NMI" pad="142"/>
<connect gate="G$1" pin="!RD" pad="95"/>
<connect gate="G$1" pin="!READY" pad="97"/>
<connect gate="G$1" pin="!RSTIN" pad="140"/>
<connect gate="G$1" pin="!RSTOUT" pad="141"/>
<connect gate="G$1" pin="!WR!/!WRL" pad="96"/>
<connect gate="G$1" pin="ALE" pad="98"/>
<connect gate="G$1" pin="P0H-0" pad="108"/>
<connect gate="G$1" pin="P0H-1" pad="111"/>
<connect gate="G$1" pin="P0H-2" pad="112"/>
<connect gate="G$1" pin="P0H-3" pad="113"/>
<connect gate="G$1" pin="P0H-4" pad="114"/>
<connect gate="G$1" pin="P0H-5" pad="115"/>
<connect gate="G$1" pin="P0H-6" pad="116"/>
<connect gate="G$1" pin="P0H-7" pad="117"/>
<connect gate="G$1" pin="P0L-0" pad="100"/>
<connect gate="G$1" pin="P0L-1" pad="101"/>
<connect gate="G$1" pin="P0L-2" pad="102"/>
<connect gate="G$1" pin="P0L-3" pad="103"/>
<connect gate="G$1" pin="P0L-4" pad="104"/>
<connect gate="G$1" pin="P0L-5" pad="105"/>
<connect gate="G$1" pin="P0L-6" pad="106"/>
<connect gate="G$1" pin="P0L-7" pad="107"/>
<connect gate="G$1" pin="P1H-0" pad="128"/>
<connect gate="G$1" pin="P1H-1" pad="129"/>
<connect gate="G$1" pin="P1H-2" pad="130"/>
<connect gate="G$1" pin="P1H-3" pad="131"/>
<connect gate="G$1" pin="P1H-4" pad="132"/>
<connect gate="G$1" pin="P1H-5" pad="133"/>
<connect gate="G$1" pin="P1H-6" pad="134"/>
<connect gate="G$1" pin="P1H-7" pad="135"/>
<connect gate="G$1" pin="P1L-0" pad="118"/>
<connect gate="G$1" pin="P1L-1" pad="119"/>
<connect gate="G$1" pin="P1L-2" pad="120"/>
<connect gate="G$1" pin="P1L-3" pad="121"/>
<connect gate="G$1" pin="P1L-4" pad="122"/>
<connect gate="G$1" pin="P1L-5" pad="123"/>
<connect gate="G$1" pin="P1L-6" pad="124"/>
<connect gate="G$1" pin="P1L-7" pad="125"/>
<connect gate="G$1" pin="P2-0" pad="47"/>
<connect gate="G$1" pin="P2-1" pad="48"/>
<connect gate="G$1" pin="P2-10" pad="59"/>
<connect gate="G$1" pin="P2-11" pad="60"/>
<connect gate="G$1" pin="P2-12" pad="61"/>
<connect gate="G$1" pin="P2-13" pad="62"/>
<connect gate="G$1" pin="P2-14" pad="63"/>
<connect gate="G$1" pin="P2-15" pad="64"/>
<connect gate="G$1" pin="P2-2" pad="49"/>
<connect gate="G$1" pin="P2-3" pad="50"/>
<connect gate="G$1" pin="P2-4" pad="51"/>
<connect gate="G$1" pin="P2-5" pad="52"/>
<connect gate="G$1" pin="P2-6" pad="53"/>
<connect gate="G$1" pin="P2-7" pad="54"/>
<connect gate="G$1" pin="P2-8" pad="57"/>
<connect gate="G$1" pin="P2-9" pad="58"/>
<connect gate="G$1" pin="P3-0" pad="65"/>
<connect gate="G$1" pin="P3-1" pad="66"/>
<connect gate="G$1" pin="P3-10" pad="77"/>
<connect gate="G$1" pin="P3-11" pad="78"/>
<connect gate="G$1" pin="P3-12" pad="79"/>
<connect gate="G$1" pin="P3-13" pad="80"/>
<connect gate="G$1" pin="P3-15" pad="81"/>
<connect gate="G$1" pin="P3-2" pad="67"/>
<connect gate="G$1" pin="P3-3" pad="68"/>
<connect gate="G$1" pin="P3-4" pad="69"/>
<connect gate="G$1" pin="P3-5" pad="70"/>
<connect gate="G$1" pin="P3-6" pad="73"/>
<connect gate="G$1" pin="P3-7" pad="74"/>
<connect gate="G$1" pin="P3-8" pad="75"/>
<connect gate="G$1" pin="P3-9" pad="76"/>
<connect gate="G$1" pin="P4-0" pad="85"/>
<connect gate="G$1" pin="P4-1" pad="86"/>
<connect gate="G$1" pin="P4-2" pad="87"/>
<connect gate="G$1" pin="P4-3" pad="88"/>
<connect gate="G$1" pin="P4-4" pad="89"/>
<connect gate="G$1" pin="P4-5" pad="90"/>
<connect gate="G$1" pin="P4-6" pad="91"/>
<connect gate="G$1" pin="P4-7" pad="92"/>
<connect gate="G$1" pin="P5-0" pad="27"/>
<connect gate="G$1" pin="P5-1" pad="28"/>
<connect gate="G$1" pin="P5-10" pad="39"/>
<connect gate="G$1" pin="P5-11" pad="40"/>
<connect gate="G$1" pin="P5-12" pad="41"/>
<connect gate="G$1" pin="P5-13" pad="42"/>
<connect gate="G$1" pin="P5-14" pad="43"/>
<connect gate="G$1" pin="P5-15" pad="44"/>
<connect gate="G$1" pin="P5-2" pad="29"/>
<connect gate="G$1" pin="P5-3" pad="30"/>
<connect gate="G$1" pin="P5-4" pad="31"/>
<connect gate="G$1" pin="P5-5" pad="32"/>
<connect gate="G$1" pin="P5-6" pad="33"/>
<connect gate="G$1" pin="P5-7" pad="34"/>
<connect gate="G$1" pin="P5-8" pad="35"/>
<connect gate="G$1" pin="P5-9" pad="36"/>
<connect gate="G$1" pin="P6-0" pad="1"/>
<connect gate="G$1" pin="P6-1" pad="2"/>
<connect gate="G$1" pin="P6-2" pad="3"/>
<connect gate="G$1" pin="P6-3" pad="4"/>
<connect gate="G$1" pin="P6-4" pad="5"/>
<connect gate="G$1" pin="P6-5" pad="6"/>
<connect gate="G$1" pin="P6-6" pad="7"/>
<connect gate="G$1" pin="P6-7" pad="8"/>
<connect gate="G$1" pin="P7-0" pad="19"/>
<connect gate="G$1" pin="P7-1" pad="20"/>
<connect gate="G$1" pin="P7-2" pad="21"/>
<connect gate="G$1" pin="P7-3" pad="22"/>
<connect gate="G$1" pin="P7-4" pad="23"/>
<connect gate="G$1" pin="P7-5" pad="24"/>
<connect gate="G$1" pin="P7-6" pad="25"/>
<connect gate="G$1" pin="P7-7" pad="26"/>
<connect gate="G$1" pin="P8-0" pad="9"/>
<connect gate="G$1" pin="P8-1" pad="10"/>
<connect gate="G$1" pin="P8-2" pad="11"/>
<connect gate="G$1" pin="P8-3" pad="12"/>
<connect gate="G$1" pin="P8-4" pad="13"/>
<connect gate="G$1" pin="P8-5" pad="14"/>
<connect gate="G$1" pin="P8-6" pad="15"/>
<connect gate="G$1" pin="P8-7" pad="16"/>
<connect gate="G$1" pin="VAGND" pad="38"/>
<connect gate="G$1" pin="VAREF" pad="37"/>
<connect gate="G$1" pin="VPP" pad="84"/>
<connect gate="G$1" pin="XTAL1" pad="138"/>
<connect gate="G$1" pin="XTAL2" pad="137"/>
<connect gate="P" pin="VCC@1" pad="17"/>
<connect gate="P" pin="VCC@10" pad="144"/>
<connect gate="P" pin="VCC@2" pad="46"/>
<connect gate="P" pin="VCC@3" pad="56"/>
<connect gate="P" pin="VCC@4" pad="72"/>
<connect gate="P" pin="VCC@5" pad="82"/>
<connect gate="P" pin="VCC@6" pad="93"/>
<connect gate="P" pin="VCC@7" pad="109"/>
<connect gate="P" pin="VCC@8" pad="126"/>
<connect gate="P" pin="VCC@9" pad="136"/>
<connect gate="P" pin="VSS@1" pad="18"/>
<connect gate="P" pin="VSS@10" pad="143"/>
<connect gate="P" pin="VSS@2" pad="45"/>
<connect gate="P" pin="VSS@3" pad="55"/>
<connect gate="P" pin="VSS@4" pad="71"/>
<connect gate="P" pin="VSS@5" pad="83"/>
<connect gate="P" pin="VSS@6" pad="94"/>
<connect gate="P" pin="VSS@7" pad="110"/>
<connect gate="P" pin="VSS@8" pad="127"/>
<connect gate="P" pin="VSS@9" pad="139"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SAK-C167CR-LM HA"/>
<attribute name="OC_FARNELL" value="1220083"/>
<attribute name="OC_NEWARK" value="24M7191"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA*-C167CR-LM" prefix="IC" uservalue="yes">
<description>16bit Microcontroller</description>
<gates>
<gate name="G" symbol="C167-1-1"/>
<gate name="P" symbol="10VCCVSS-1"/>
</gates>
<devices>
<device name="" package="MQFP144-RND">
<connects>
<connect gate="G" pin="!EA" pad="99"/>
<connect gate="G" pin="!NMI" pad="142"/>
<connect gate="G" pin="!RD" pad="95"/>
<connect gate="G" pin="!READY" pad="97"/>
<connect gate="G" pin="!RSTIN" pad="140"/>
<connect gate="G" pin="!RSTOUT" pad="141"/>
<connect gate="G" pin="!WR!/!WRL" pad="96"/>
<connect gate="G" pin="ALE" pad="98"/>
<connect gate="G" pin="P.0/AN0" pad="27"/>
<connect gate="G" pin="P0.0/AD0" pad="100"/>
<connect gate="G" pin="P0.1/AD1" pad="101"/>
<connect gate="G" pin="P0.10/AD10" pad="112"/>
<connect gate="G" pin="P0.11/AD11" pad="113"/>
<connect gate="G" pin="P0.12/AD12" pad="114"/>
<connect gate="G" pin="P0.13/AD13" pad="115"/>
<connect gate="G" pin="P0.14/AD14" pad="116"/>
<connect gate="G" pin="P0.15/AD15" pad="117"/>
<connect gate="G" pin="P0.2/AD2" pad="102"/>
<connect gate="G" pin="P0.3/AD3" pad="103"/>
<connect gate="G" pin="P0.4/AD4" pad="104"/>
<connect gate="G" pin="P0.5/AD5" pad="105"/>
<connect gate="G" pin="P0.6/AD6" pad="106"/>
<connect gate="G" pin="P0.7/AD7" pad="107"/>
<connect gate="G" pin="P0.8/AD8" pad="108"/>
<connect gate="G" pin="P0.9/AD9" pad="111"/>
<connect gate="G" pin="P1.0" pad="118"/>
<connect gate="G" pin="P1.1" pad="119"/>
<connect gate="G" pin="P1.10" pad="130"/>
<connect gate="G" pin="P1.11" pad="131"/>
<connect gate="G" pin="P1.2" pad="120"/>
<connect gate="G" pin="P1.3" pad="121"/>
<connect gate="G" pin="P1.4" pad="122"/>
<connect gate="G" pin="P1.4/CC24" pad="132"/>
<connect gate="G" pin="P1.5" pad="123"/>
<connect gate="G" pin="P1.5/CC25" pad="133"/>
<connect gate="G" pin="P1.6" pad="124"/>
<connect gate="G" pin="P1.6/CC26" pad="134"/>
<connect gate="G" pin="P1.7" pad="125"/>
<connect gate="G" pin="P1.7/CC27" pad="135"/>
<connect gate="G" pin="P1.8" pad="128"/>
<connect gate="G" pin="P1.9" pad="129"/>
<connect gate="G" pin="P2.0/CC0IO" pad="47"/>
<connect gate="G" pin="P2.1/CC1IO" pad="48"/>
<connect gate="G" pin="P2.10/EX2I" pad="59"/>
<connect gate="G" pin="P2.11/EX3I" pad="60"/>
<connect gate="G" pin="P2.12/EX4I" pad="61"/>
<connect gate="G" pin="P2.13/EX5I" pad="62"/>
<connect gate="G" pin="P2.14/EX6I" pad="63"/>
<connect gate="G" pin="P2.15/EX7I" pad="64"/>
<connect gate="G" pin="P2.2/CC2IO" pad="49"/>
<connect gate="G" pin="P2.3/CC3IO" pad="50"/>
<connect gate="G" pin="P2.4/CC4IO" pad="51"/>
<connect gate="G" pin="P2.5/CC5IO" pad="52"/>
<connect gate="G" pin="P2.6/CC6IO" pad="53"/>
<connect gate="G" pin="P2.7/CC7IO" pad="54"/>
<connect gate="G" pin="P2.8/EX0IN" pad="57"/>
<connect gate="G" pin="P2.9/EX1IN" pad="58"/>
<connect gate="G" pin="P3.0/T0IN" pad="65"/>
<connect gate="G" pin="P3.1/T6OUT" pad="66"/>
<connect gate="G" pin="P3.10/TXD0" pad="77"/>
<connect gate="G" pin="P3.11/RXD0" pad="78"/>
<connect gate="G" pin="P3.12/BHE" pad="79"/>
<connect gate="G" pin="P3.13/SCLK" pad="80"/>
<connect gate="G" pin="P3.15/CLKO" pad="81"/>
<connect gate="G" pin="P3.2/CAPIN" pad="67"/>
<connect gate="G" pin="P3.3/T3OUT" pad="68"/>
<connect gate="G" pin="P3.4/T3EUD" pad="69"/>
<connect gate="G" pin="P3.5/T4IN" pad="70"/>
<connect gate="G" pin="P3.6/T3IN" pad="73"/>
<connect gate="G" pin="P3.7/T2IN" pad="74"/>
<connect gate="G" pin="P3.8/MRST" pad="75"/>
<connect gate="G" pin="P3.9/MTSR" pad="76"/>
<connect gate="G" pin="P4.0/A16" pad="85"/>
<connect gate="G" pin="P4.1/A17" pad="86"/>
<connect gate="G" pin="P4.2/A18" pad="87"/>
<connect gate="G" pin="P4.3/A19" pad="88"/>
<connect gate="G" pin="P4.4/A20" pad="89"/>
<connect gate="G" pin="P4.5/A21" pad="90"/>
<connect gate="G" pin="P4.6/A22" pad="91"/>
<connect gate="G" pin="P4.7/A23" pad="92"/>
<connect gate="G" pin="P5.1/AN1" pad="28"/>
<connect gate="G" pin="P5.10/AN10" pad="39"/>
<connect gate="G" pin="P5.11/AN11" pad="40"/>
<connect gate="G" pin="P5.12/AN12" pad="41"/>
<connect gate="G" pin="P5.13/AN13" pad="42"/>
<connect gate="G" pin="P5.14/AN14" pad="43"/>
<connect gate="G" pin="P5.15/AN15" pad="44"/>
<connect gate="G" pin="P5.2/AN2" pad="29"/>
<connect gate="G" pin="P5.3/AN3" pad="30"/>
<connect gate="G" pin="P5.4/AN4" pad="31"/>
<connect gate="G" pin="P5.5/AN5" pad="32"/>
<connect gate="G" pin="P5.6/AN6" pad="33"/>
<connect gate="G" pin="P5.7/AN7" pad="34"/>
<connect gate="G" pin="P5.8/AN8" pad="35"/>
<connect gate="G" pin="P5.9/AN9" pad="36"/>
<connect gate="G" pin="P6.0/CS0" pad="1"/>
<connect gate="G" pin="P6.1/CS1" pad="2"/>
<connect gate="G" pin="P6.2/CS2" pad="3"/>
<connect gate="G" pin="P6.3/CS3" pad="4"/>
<connect gate="G" pin="P6.4/CS4" pad="5"/>
<connect gate="G" pin="P6.5/HOLD" pad="6"/>
<connect gate="G" pin="P6.6/HLDA" pad="7"/>
<connect gate="G" pin="P6.7/BREQ" pad="8"/>
<connect gate="G" pin="P7.0/POUT0" pad="19"/>
<connect gate="G" pin="P7.1/POUT1" pad="20"/>
<connect gate="G" pin="P7.2/POUT2" pad="21"/>
<connect gate="G" pin="P7.3/POUT3" pad="22"/>
<connect gate="G" pin="P7.4CC28IO" pad="23"/>
<connect gate="G" pin="P7.5CC29IO" pad="24"/>
<connect gate="G" pin="P7.6CC30IO" pad="25"/>
<connect gate="G" pin="P7.7CC31IO" pad="26"/>
<connect gate="G" pin="P8.0CC16IO" pad="9"/>
<connect gate="G" pin="P8.1CC17IO" pad="10"/>
<connect gate="G" pin="P8.2CC18IO" pad="11"/>
<connect gate="G" pin="P8.3CC19IO" pad="12"/>
<connect gate="G" pin="P8.4CC20IO" pad="13"/>
<connect gate="G" pin="P8.5CC21IO" pad="14"/>
<connect gate="G" pin="P8.6CC22IO" pad="15"/>
<connect gate="G" pin="P8.7CC23IO" pad="16"/>
<connect gate="G" pin="VAGND" pad="38"/>
<connect gate="G" pin="VAREF" pad="37"/>
<connect gate="G" pin="VPP" pad="84"/>
<connect gate="G" pin="XTAL1" pad="138"/>
<connect gate="G" pin="XTAL2" pad="137"/>
<connect gate="P" pin="VCC@1" pad="17"/>
<connect gate="P" pin="VCC@10" pad="144"/>
<connect gate="P" pin="VCC@2" pad="46"/>
<connect gate="P" pin="VCC@3" pad="56"/>
<connect gate="P" pin="VCC@4" pad="72"/>
<connect gate="P" pin="VCC@5" pad="82"/>
<connect gate="P" pin="VCC@6" pad="93"/>
<connect gate="P" pin="VCC@7" pad="109"/>
<connect gate="P" pin="VCC@8" pad="126"/>
<connect gate="P" pin="VCC@9" pad="136"/>
<connect gate="P" pin="VSS@1" pad="18"/>
<connect gate="P" pin="VSS@10" pad="143"/>
<connect gate="P" pin="VSS@2" pad="45"/>
<connect gate="P" pin="VSS@3" pad="55"/>
<connect gate="P" pin="VSS@4" pad="71"/>
<connect gate="P" pin="VSS@5" pad="83"/>
<connect gate="P" pin="VSS@6" pad="94"/>
<connect gate="P" pin="VSS@7" pad="110"/>
<connect gate="P" pin="VSS@8" pad="127"/>
<connect gate="P" pin="VSS@9" pad="139"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SAK-C167CR-LM HA"/>
<attribute name="OC_FARNELL" value="1220083"/>
<attribute name="OC_NEWARK" value="24M7191"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA*-XC167" prefix="IC">
<description>&lt;b&gt;16-Bit Single-Chip Microcontroller&lt;/b&gt;&lt;p&gt;
Source: xc167_ds_v1.1_2003_06.pdf</description>
<gates>
<gate name="-POWER" symbol="XC167-POWER"/>
<gate name="-BUS-INTERFACE" symbol="XC167-BUS"/>
<gate name="-CLOCK-JTAG-OCDSI" symbol="XC167-CLOCK-JTAG"/>
<gate name="-PORTS" symbol="XC167-PORTS"/>
</gates>
<devices>
<device name="P" package="P-TQFP-144-19">
<connects>
<connect gate="-BUS-INTERFACE" pin="/NMI" pad="4"/>
<connect gate="-BUS-INTERFACE" pin="/RSTIN" pad="142"/>
<connect gate="-BUS-INTERFACE" pin="P0H.0-AD8" pad="105"/>
<connect gate="-BUS-INTERFACE" pin="P0H.1-AD9" pad="106"/>
<connect gate="-BUS-INTERFACE" pin="P0H.2-AD10" pad="111"/>
<connect gate="-BUS-INTERFACE" pin="P0H.3-AD11" pad="112"/>
<connect gate="-BUS-INTERFACE" pin="P0H.4-AD12" pad="113"/>
<connect gate="-BUS-INTERFACE" pin="P0H.5-AD13" pad="114"/>
<connect gate="-BUS-INTERFACE" pin="P0H.6-AD14" pad="115"/>
<connect gate="-BUS-INTERFACE" pin="P0H.7-AD15" pad="116"/>
<connect gate="-BUS-INTERFACE" pin="P0L.0-AD0" pad="95"/>
<connect gate="-BUS-INTERFACE" pin="P0L.1-AD1" pad="96"/>
<connect gate="-BUS-INTERFACE" pin="P0L.2-AD2" pad="97"/>
<connect gate="-BUS-INTERFACE" pin="P0L.3-AD3" pad="98"/>
<connect gate="-BUS-INTERFACE" pin="P0L.4-AD4" pad="99"/>
<connect gate="-BUS-INTERFACE" pin="P0L.5-AD5" pad="100"/>
<connect gate="-BUS-INTERFACE" pin="P0L.6-AD6" pad="101"/>
<connect gate="-BUS-INTERFACE" pin="P0L.7-AD7" pad="102"/>
<connect gate="-BUS-INTERFACE" pin="P1H.0-A8-/C6P0-CC23-E*" pad="127"/>
<connect gate="-BUS-INTERFACE" pin="P1H.1-A9-/C6P1-MRST1" pad="128"/>
<connect gate="-BUS-INTERFACE" pin="P1H.2-A10-/C6P2-MTSR1" pad="129"/>
<connect gate="-BUS-INTERFACE" pin="P1H.3-A11-SCLK1-E*" pad="130"/>
<connect gate="-BUS-INTERFACE" pin="P1H.4-A12-CC24IO" pad="131"/>
<connect gate="-BUS-INTERFACE" pin="P1H.5-A13-CC25IO" pad="132"/>
<connect gate="-BUS-INTERFACE" pin="P1H.6-A14-CC26IO" pad="133"/>
<connect gate="-BUS-INTERFACE" pin="P1H.7-A15-CC27IO" pad="134"/>
<connect gate="-BUS-INTERFACE" pin="P1L.0-A0-CC60" pad="117"/>
<connect gate="-BUS-INTERFACE" pin="P1L.1-A1-COUT60" pad="118"/>
<connect gate="-BUS-INTERFACE" pin="P1L.2-A2-CC61" pad="119"/>
<connect gate="-BUS-INTERFACE" pin="P1L.3-A3-COUT61" pad="120"/>
<connect gate="-BUS-INTERFACE" pin="P1L.4-A4-CC62" pad="121"/>
<connect gate="-BUS-INTERFACE" pin="P1L.5-A5-COUT62" pad="122"/>
<connect gate="-BUS-INTERFACE" pin="P1L.6-A6-COUT63" pad="123"/>
<connect gate="-BUS-INTERFACE" pin="P1L.7-A7-/CTRAP-CC22" pad="124"/>
<connect gate="-BUS-INTERFACE" pin="P20.0-/RD" pad="90"/>
<connect gate="-BUS-INTERFACE" pin="P20.1-/WR-/WRL" pad="91"/>
<connect gate="-BUS-INTERFACE" pin="P20.12-/RSTOUT" pad="3"/>
<connect gate="-BUS-INTERFACE" pin="P20.2-READY" pad="92"/>
<connect gate="-BUS-INTERFACE" pin="P20.4-ALE" pad="93"/>
<connect gate="-BUS-INTERFACE" pin="P20.5-/EA" pad="94"/>
<connect gate="-BUS-INTERFACE" pin="P3.12-/BHE-/WRH" pad="75"/>
<connect gate="-BUS-INTERFACE" pin="P4.0-A16" pad="80"/>
<connect gate="-BUS-INTERFACE" pin="P4.1-A17" pad="81"/>
<connect gate="-BUS-INTERFACE" pin="P4.2-A18" pad="82"/>
<connect gate="-BUS-INTERFACE" pin="P4.3-A19" pad="83"/>
<connect gate="-BUS-INTERFACE" pin="P4.4-A20-C*" pad="84"/>
<connect gate="-BUS-INTERFACE" pin="P4.5-A21-C*" pad="85"/>
<connect gate="-BUS-INTERFACE" pin="P4.6-A22-C*" pad="86"/>
<connect gate="-BUS-INTERFACE" pin="P4.7-A23-C*" pad="87"/>
<connect gate="-BUS-INTERFACE" pin="P6.0-/CS0-CC0IO" pad="7"/>
<connect gate="-BUS-INTERFACE" pin="P6.1-/CS1-CC1IO" pad="8"/>
<connect gate="-BUS-INTERFACE" pin="P6.2-/CS2-CC2IO" pad="9"/>
<connect gate="-BUS-INTERFACE" pin="P6.3-/CS3-CC3IO" pad="10"/>
<connect gate="-BUS-INTERFACE" pin="P6.4-/CS4-CC4IO" pad="11"/>
<connect gate="-BUS-INTERFACE" pin="P6.5-/HOLD-CC5IO" pad="12"/>
<connect gate="-BUS-INTERFACE" pin="P6.6-/HLDA-CC6IO" pad="13"/>
<connect gate="-BUS-INTERFACE" pin="P6.7-/BREQ-CC7IO" pad="14"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="/BRKIN" pad="144"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="/BRKOUT" pad="143"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="/TRST" pad="57"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="P3.15-CLKOUT-F" pad="77"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="TCK" pad="71"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="TDI" pad="72"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="TDO" pad="73"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="TMS-E*" pad="74"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="XTAL1" pad="138"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="XTAL2" pad="137"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="XTAL3" pad="140"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="XTAL4" pad="141"/>
<connect gate="-PORTS" pin="P2.10-CC10IO-EX2IN" pad="51"/>
<connect gate="-PORTS" pin="P2.11-CC11IO-EX3IN" pad="52"/>
<connect gate="-PORTS" pin="P2.12-CC12IO-EX4IN" pad="53"/>
<connect gate="-PORTS" pin="P2.13-CC13IO-EX5IN" pad="54"/>
<connect gate="-PORTS" pin="P2.14-CC14IO-EX6IN" pad="55"/>
<connect gate="-PORTS" pin="P2.15-CC15IO-EX7IN-T7IN" pad="56"/>
<connect gate="-PORTS" pin="P2.8-CC8IO-EX0IN" pad="49"/>
<connect gate="-PORTS" pin="P2.9-CC9IO-EX1IN" pad="50"/>
<connect gate="-PORTS" pin="P3.0-T0IN-TXD1-E*" pad="59"/>
<connect gate="-PORTS" pin="P3.1-T6OUT-RXD1-E*" pad="60"/>
<connect gate="-PORTS" pin="P3.10-TXD0-E*" pad="69"/>
<connect gate="-PORTS" pin="P3.11-RXD0-E*" pad="70"/>
<connect gate="-PORTS" pin="P3.13-SCLK0-E*" pad="76"/>
<connect gate="-PORTS" pin="P3.2-CAPIN" pad="61"/>
<connect gate="-PORTS" pin="P3.3-T3OUT" pad="62"/>
<connect gate="-PORTS" pin="P3.4-T3EUD" pad="63"/>
<connect gate="-PORTS" pin="P3.5-T4IN" pad="64"/>
<connect gate="-PORTS" pin="P3.6-T3IN" pad="65"/>
<connect gate="-PORTS" pin="P3.7-T2IN" pad="66"/>
<connect gate="-PORTS" pin="P3.8-MRST0" pad="67"/>
<connect gate="-PORTS" pin="P3.9-MTSR0" pad="68"/>
<connect gate="-PORTS" pin="P5.0-AN0" pad="29"/>
<connect gate="-PORTS" pin="P5.1-AN1" pad="30"/>
<connect gate="-PORTS" pin="P5.10-AN10-T6EUD" pad="35"/>
<connect gate="-PORTS" pin="P5.11-AN11-T5EUD" pad="36"/>
<connect gate="-PORTS" pin="P5.12-AN12-T6IN" pad="43"/>
<connect gate="-PORTS" pin="P5.13-AN13-T5IN" pad="44"/>
<connect gate="-PORTS" pin="P5.14-AN14-T4EUD" pad="45"/>
<connect gate="-PORTS" pin="P5.15-AN15-T2EUD" pad="46"/>
<connect gate="-PORTS" pin="P5.2-AN2" pad="31"/>
<connect gate="-PORTS" pin="P5.3-AN3" pad="32"/>
<connect gate="-PORTS" pin="P5.4-AN4" pad="33"/>
<connect gate="-PORTS" pin="P5.5-AN5" pad="34"/>
<connect gate="-PORTS" pin="P5.6-AN6" pad="39"/>
<connect gate="-PORTS" pin="P5.7-AN7" pad="40"/>
<connect gate="-PORTS" pin="P5.8-AN8" pad="37"/>
<connect gate="-PORTS" pin="P5.9-AN9" pad="38"/>
<connect gate="-PORTS" pin="P7.4-CC28IO-C*" pad="15"/>
<connect gate="-PORTS" pin="P7.5-CC29IO-C*" pad="16"/>
<connect gate="-PORTS" pin="P7.6-CC30IO-C*" pad="17"/>
<connect gate="-PORTS" pin="P7.7-CC31IO-C*" pad="18"/>
<connect gate="-PORTS" pin="P9.0-SDA0-CC16IO-C*" pad="21"/>
<connect gate="-PORTS" pin="P9.1-SCL0-CC17IO-C*" pad="22"/>
<connect gate="-PORTS" pin="P9.2-SDA1-CC18IO-C*" pad="23"/>
<connect gate="-PORTS" pin="P9.3-SCL1-CC19IO-C*" pad="24"/>
<connect gate="-PORTS" pin="P9.4-SDA2-CC20IO" pad="25"/>
<connect gate="-PORTS" pin="P9.5-SCL2-CC21IO" pad="26"/>
<connect gate="-PORTS" pin="VAGND" pad="42"/>
<connect gate="-PORTS" pin="VAREF" pad="41"/>
<connect gate="-POWER" pin="VDDI" pad="135"/>
<connect gate="-POWER" pin="VDDI@1" pad="78"/>
<connect gate="-POWER" pin="VDDI@2" pad="48"/>
<connect gate="-POWER" pin="VDDP" pad="125"/>
<connect gate="-POWER" pin="VDDP@1" pad="103"/>
<connect gate="-POWER" pin="VDDP@2" pad="88"/>
<connect gate="-POWER" pin="VDDP@3" pad="58"/>
<connect gate="-POWER" pin="VDDP@4" pad="28"/>
<connect gate="-POWER" pin="VDDP@5" pad="20"/>
<connect gate="-POWER" pin="VDDP@6" pad="6"/>
<connect gate="-POWER" pin="VSSI" pad="136"/>
<connect gate="-POWER" pin="VSSI@1" pad="139"/>
<connect gate="-POWER" pin="VSSI@2" pad="79"/>
<connect gate="-POWER" pin="VSSI@3" pad="47"/>
<connect gate="-POWER" pin="VSSP" pad="126"/>
<connect gate="-POWER" pin="VSSP@1" pad="104"/>
<connect gate="-POWER" pin="VSSP@2" pad="89"/>
<connect gate="-POWER" pin="VSSP@3" pad="27"/>
<connect gate="-POWER" pin="VSSP@4" pad="19"/>
<connect gate="-POWER" pin="VSSP@5" pad="5"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA*-XC167CI" prefix="IC">
<description>16bit Microcontroller with MAC Unit 256KB Flash</description>
<gates>
<gate name="G" symbol="XC167CI"/>
</gates>
<devices>
<device name="" package="P-TQFP144">
<connects>
<connect gate="G" pin="/BRKIN" pad="144"/>
<connect gate="G" pin="/BRKOUT" pad="143"/>
<connect gate="G" pin="/EA-P20.5" pad="94"/>
<connect gate="G" pin="/NMI" pad="4"/>
<connect gate="G" pin="/RESET-IN" pad="142"/>
<connect gate="G" pin="/RESET-OUT" pad="3"/>
<connect gate="G" pin="/TRST" pad="57"/>
<connect gate="G" pin="NC@0" pad="1"/>
<connect gate="G" pin="NC@1" pad="2"/>
<connect gate="G" pin="NC@2" pad="107"/>
<connect gate="G" pin="NC@3" pad="108"/>
<connect gate="G" pin="NC@4" pad="109"/>
<connect gate="G" pin="NC@5" pad="110"/>
<connect gate="G" pin="P0H.0-AD8" pad="105"/>
<connect gate="G" pin="P0H.1-AD9" pad="106"/>
<connect gate="G" pin="P0H.2-AD10" pad="111"/>
<connect gate="G" pin="P0H.3-AD11" pad="112"/>
<connect gate="G" pin="P0H.4-AD12" pad="113"/>
<connect gate="G" pin="P0H.5-AD13" pad="114"/>
<connect gate="G" pin="P0H.6-AD14" pad="115"/>
<connect gate="G" pin="P0H.7-AD15" pad="116"/>
<connect gate="G" pin="P0L.0-AD0" pad="95"/>
<connect gate="G" pin="P0L.1-AD1" pad="96"/>
<connect gate="G" pin="P0L.2-AD2" pad="97"/>
<connect gate="G" pin="P0L.3-AD3" pad="98"/>
<connect gate="G" pin="P0L.4-AD4" pad="99"/>
<connect gate="G" pin="P0L.5-AD5" pad="100"/>
<connect gate="G" pin="P0L.6-AD6" pad="101"/>
<connect gate="G" pin="P0L.7-AD7" pad="102"/>
<connect gate="G" pin="P1H.0-A8" pad="127"/>
<connect gate="G" pin="P1H.1-A9" pad="128"/>
<connect gate="G" pin="P1H.2-A10" pad="129"/>
<connect gate="G" pin="P1H.3-A11" pad="130"/>
<connect gate="G" pin="P1H.4-A12" pad="131"/>
<connect gate="G" pin="P1H.5-A13" pad="132"/>
<connect gate="G" pin="P1H.6-A14" pad="133"/>
<connect gate="G" pin="P1H.7-A15" pad="134"/>
<connect gate="G" pin="P1L.0-A0" pad="117"/>
<connect gate="G" pin="P1L.1-A1" pad="118"/>
<connect gate="G" pin="P1L.2-A2" pad="119"/>
<connect gate="G" pin="P1L.3-A3" pad="120"/>
<connect gate="G" pin="P1L.4-A4" pad="121"/>
<connect gate="G" pin="P1L.5-A5" pad="122"/>
<connect gate="G" pin="P1L.6-A6" pad="123"/>
<connect gate="G" pin="P1L.7-A7" pad="124"/>
<connect gate="G" pin="P2.10-CC10IO-EX2IN" pad="51"/>
<connect gate="G" pin="P2.11-CC11IO-EX3IN" pad="52"/>
<connect gate="G" pin="P2.12-CC12IO-EX4IN" pad="53"/>
<connect gate="G" pin="P2.13-CC13IO-EX5IN" pad="54"/>
<connect gate="G" pin="P2.14-CC14IO-EX6IN" pad="55"/>
<connect gate="G" pin="P2.15-CC15IO-EX7IN-T7IN" pad="56"/>
<connect gate="G" pin="P2.8-CC8IO-EX0IN" pad="49"/>
<connect gate="G" pin="P2.9-CC9IO-EX1IN" pad="50"/>
<connect gate="G" pin="P20.0-/RD" pad="90"/>
<connect gate="G" pin="P20.1-/WR-/WRL" pad="91"/>
<connect gate="G" pin="P20.2-READY" pad="92"/>
<connect gate="G" pin="P20.4-ALE" pad="93"/>
<connect gate="G" pin="P3.0-T0IN-TXD1-E*" pad="59"/>
<connect gate="G" pin="P3.1-T6OUT-RXD0-E*" pad="60"/>
<connect gate="G" pin="P3.10-TXD0-E*" pad="69"/>
<connect gate="G" pin="P3.11-RXD0-E*" pad="70"/>
<connect gate="G" pin="P3.12-/BHE-/WRH" pad="75"/>
<connect gate="G" pin="P3.13-SCLK0-E*" pad="76"/>
<connect gate="G" pin="P3.15-CLKOUT-F" pad="77"/>
<connect gate="G" pin="P3.2-CAPIN" pad="61"/>
<connect gate="G" pin="P3.3-T3OUT" pad="62"/>
<connect gate="G" pin="P3.4-T3EUD" pad="63"/>
<connect gate="G" pin="P3.5-T4IN" pad="64"/>
<connect gate="G" pin="P3.6-T3IN" pad="65"/>
<connect gate="G" pin="P3.7-T2IN" pad="66"/>
<connect gate="G" pin="P3.8-MRST0" pad="67"/>
<connect gate="G" pin="P3.9-MTSR0" pad="68"/>
<connect gate="G" pin="P4.0-A16" pad="80"/>
<connect gate="G" pin="P4.1-A17" pad="81"/>
<connect gate="G" pin="P4.2-A18" pad="82"/>
<connect gate="G" pin="P4.3-A19" pad="83"/>
<connect gate="G" pin="P4.4-A20-C*" pad="84"/>
<connect gate="G" pin="P4.5-A21-C*" pad="85"/>
<connect gate="G" pin="P4.6-A22-C*" pad="86"/>
<connect gate="G" pin="P4.7-A23-C*" pad="87"/>
<connect gate="G" pin="P5.0-AN0" pad="29"/>
<connect gate="G" pin="P5.1-AN1" pad="30"/>
<connect gate="G" pin="P5.10-AN10" pad="35"/>
<connect gate="G" pin="P5.11-AN11" pad="36"/>
<connect gate="G" pin="P5.12-AN12" pad="43"/>
<connect gate="G" pin="P5.13-AN13" pad="44"/>
<connect gate="G" pin="P5.14-AN14" pad="45"/>
<connect gate="G" pin="P5.15-AN15" pad="46"/>
<connect gate="G" pin="P5.2-AN2" pad="31"/>
<connect gate="G" pin="P5.3-AN3" pad="32"/>
<connect gate="G" pin="P5.4-AN4" pad="33"/>
<connect gate="G" pin="P5.5-AN5" pad="34"/>
<connect gate="G" pin="P5.6-AN6" pad="39"/>
<connect gate="G" pin="P5.7-AN7" pad="40"/>
<connect gate="G" pin="P5.8-AN8" pad="37"/>
<connect gate="G" pin="P5.9-AN9" pad="38"/>
<connect gate="G" pin="P6.0-/CS0-CC0IO" pad="7"/>
<connect gate="G" pin="P6.1-/CS1-CC1IO" pad="8"/>
<connect gate="G" pin="P6.2-/CS2-CC2IO" pad="9"/>
<connect gate="G" pin="P6.3-/CS3-CC3IO" pad="10"/>
<connect gate="G" pin="P6.4-/CS4-CC4IO" pad="11"/>
<connect gate="G" pin="P6.5-/HOLD-CC5IO" pad="12"/>
<connect gate="G" pin="P6.6-/HLDA-CC6IO" pad="13"/>
<connect gate="G" pin="P6.7-/BREQ-CC7IO" pad="14"/>
<connect gate="G" pin="P7.4-CC28IO-C*" pad="15"/>
<connect gate="G" pin="P7.5-CC29IO-C*" pad="16"/>
<connect gate="G" pin="P7.6-CC30IO-C*" pad="17"/>
<connect gate="G" pin="P7.7-CC31IO-C*" pad="18"/>
<connect gate="G" pin="P9.0-SDA0-CC16IO-C*" pad="21"/>
<connect gate="G" pin="P9.1-SCL0-CC17IO-C*" pad="22"/>
<connect gate="G" pin="P9.2-SDA1-CC18IO-C*" pad="23"/>
<connect gate="G" pin="P9.3-SCL1-CC19IO-C*" pad="24"/>
<connect gate="G" pin="P9.4-SDA2-CC20IO-C*" pad="25"/>
<connect gate="G" pin="P9.5-SCL2-CC21IO-C*" pad="26"/>
<connect gate="G" pin="TCK" pad="71"/>
<connect gate="G" pin="TDI" pad="72"/>
<connect gate="G" pin="TDO" pad="73"/>
<connect gate="G" pin="TMS-E" pad="74"/>
<connect gate="G" pin="VAGND" pad="42"/>
<connect gate="G" pin="VAREF" pad="41"/>
<connect gate="G" pin="VDDI@0" pad="135"/>
<connect gate="G" pin="VDDI@1" pad="78"/>
<connect gate="G" pin="VDDI@2" pad="48"/>
<connect gate="G" pin="VDDP@0" pad="6"/>
<connect gate="G" pin="VDDP@1" pad="20"/>
<connect gate="G" pin="VDDP@3" pad="28"/>
<connect gate="G" pin="VDDP@4" pad="58"/>
<connect gate="G" pin="VDDP@5" pad="88"/>
<connect gate="G" pin="VDDP@6" pad="103"/>
<connect gate="G" pin="VDDP@7" pad="125"/>
<connect gate="G" pin="VSSI@0" pad="47"/>
<connect gate="G" pin="VSSI@1" pad="79"/>
<connect gate="G" pin="VSSI@2" pad="139"/>
<connect gate="G" pin="VSSI@3" pad="136"/>
<connect gate="G" pin="VSSP@0" pad="5"/>
<connect gate="G" pin="VSSP@1" pad="19"/>
<connect gate="G" pin="VSSP@2" pad="27"/>
<connect gate="G" pin="VSSP@4" pad="89"/>
<connect gate="G" pin="VSSP@5" pad="104"/>
<connect gate="G" pin="VSSP@6" pad="126"/>
<connect gate="G" pin="XTAL1" pad="138"/>
<connect gate="G" pin="XTAL2" pad="137"/>
<connect gate="G" pin="XTAL3" pad="140"/>
<connect gate="G" pin="XTAL4" pad="141"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SA*C167-CR-LM" prefix="IC" uservalue="yes">
<description>16 bit Microcontroller</description>
<gates>
<gate name="G$1" symbol="C167-2"/>
<gate name="P" symbol="10VCCVSS-1"/>
</gates>
<devices>
<device name="" package="MQFP144-RND">
<connects>
<connect gate="G$1" pin="!EA" pad="99"/>
<connect gate="G$1" pin="!NMI" pad="142"/>
<connect gate="G$1" pin="!RD" pad="95"/>
<connect gate="G$1" pin="!READY" pad="97"/>
<connect gate="G$1" pin="!RSTIN" pad="140"/>
<connect gate="G$1" pin="!RSTOUT" pad="141"/>
<connect gate="G$1" pin="!WR!/!WRL" pad="96"/>
<connect gate="G$1" pin="ALE" pad="98"/>
<connect gate="G$1" pin="P.0/AN0" pad="27"/>
<connect gate="G$1" pin="P0.0/AD0" pad="100"/>
<connect gate="G$1" pin="P0.1/AD1" pad="101"/>
<connect gate="G$1" pin="P0.10/AD10" pad="112"/>
<connect gate="G$1" pin="P0.11/AD11" pad="113"/>
<connect gate="G$1" pin="P0.12/AD12" pad="114"/>
<connect gate="G$1" pin="P0.13/AD13" pad="115"/>
<connect gate="G$1" pin="P0.14/AD14" pad="116"/>
<connect gate="G$1" pin="P0.15/AD15" pad="117"/>
<connect gate="G$1" pin="P0.2/AD2" pad="102"/>
<connect gate="G$1" pin="P0.3/AD3" pad="103"/>
<connect gate="G$1" pin="P0.4/AD4" pad="104"/>
<connect gate="G$1" pin="P0.5/AD5" pad="105"/>
<connect gate="G$1" pin="P0.6/AD6" pad="106"/>
<connect gate="G$1" pin="P0.7/AD7" pad="107"/>
<connect gate="G$1" pin="P0.8/AD8" pad="108"/>
<connect gate="G$1" pin="P0.9/AD9" pad="111"/>
<connect gate="G$1" pin="P1.0" pad="118"/>
<connect gate="G$1" pin="P1.1" pad="119"/>
<connect gate="G$1" pin="P1.10" pad="130"/>
<connect gate="G$1" pin="P1.11" pad="131"/>
<connect gate="G$1" pin="P1.2" pad="120"/>
<connect gate="G$1" pin="P1.3" pad="121"/>
<connect gate="G$1" pin="P1.4" pad="122"/>
<connect gate="G$1" pin="P1.4/CC24" pad="132"/>
<connect gate="G$1" pin="P1.5" pad="123"/>
<connect gate="G$1" pin="P1.5/CC25" pad="133"/>
<connect gate="G$1" pin="P1.6" pad="124"/>
<connect gate="G$1" pin="P1.6/CC26" pad="134"/>
<connect gate="G$1" pin="P1.7" pad="125"/>
<connect gate="G$1" pin="P1.7/CC27" pad="135"/>
<connect gate="G$1" pin="P1.8" pad="128"/>
<connect gate="G$1" pin="P1.9" pad="129"/>
<connect gate="G$1" pin="P2.0/CC0IO" pad="47"/>
<connect gate="G$1" pin="P2.1/CC1IO" pad="48"/>
<connect gate="G$1" pin="P2.10/EX2I" pad="59"/>
<connect gate="G$1" pin="P2.11/EX3I" pad="60"/>
<connect gate="G$1" pin="P2.12/EX4I" pad="61"/>
<connect gate="G$1" pin="P2.13/EX5I" pad="62"/>
<connect gate="G$1" pin="P2.14/EX6I" pad="63"/>
<connect gate="G$1" pin="P2.15/EX7I" pad="64"/>
<connect gate="G$1" pin="P2.2/CC2IO" pad="49"/>
<connect gate="G$1" pin="P2.3/CC3IO" pad="50"/>
<connect gate="G$1" pin="P2.4/CC4IO" pad="51"/>
<connect gate="G$1" pin="P2.5/CC5IO" pad="52"/>
<connect gate="G$1" pin="P2.6/CC6IO" pad="53"/>
<connect gate="G$1" pin="P2.7/CC7IO" pad="54"/>
<connect gate="G$1" pin="P2.8/EX0IN" pad="57"/>
<connect gate="G$1" pin="P2.9/EX1IN" pad="58"/>
<connect gate="G$1" pin="P3.0/T0IN" pad="65"/>
<connect gate="G$1" pin="P3.1/T6OUT" pad="66"/>
<connect gate="G$1" pin="P3.10/TXD0" pad="77"/>
<connect gate="G$1" pin="P3.11/RXD0" pad="78"/>
<connect gate="G$1" pin="P3.12/BHE" pad="79"/>
<connect gate="G$1" pin="P3.13/SCLK" pad="80"/>
<connect gate="G$1" pin="P3.15/CLKO" pad="81"/>
<connect gate="G$1" pin="P3.2/CAPIN" pad="67"/>
<connect gate="G$1" pin="P3.3/T3OUT" pad="68"/>
<connect gate="G$1" pin="P3.4/T3EUD" pad="69"/>
<connect gate="G$1" pin="P3.5/T4IN" pad="70"/>
<connect gate="G$1" pin="P3.6/T3IN" pad="73"/>
<connect gate="G$1" pin="P3.7/T2IN" pad="74"/>
<connect gate="G$1" pin="P3.8/MRST" pad="75"/>
<connect gate="G$1" pin="P3.9/MTSR" pad="76"/>
<connect gate="G$1" pin="P4.0/A16" pad="85"/>
<connect gate="G$1" pin="P4.1/A17" pad="86"/>
<connect gate="G$1" pin="P4.2/A18" pad="87"/>
<connect gate="G$1" pin="P4.3/A19" pad="88"/>
<connect gate="G$1" pin="P4.4/A20" pad="89"/>
<connect gate="G$1" pin="P4.5/A21" pad="90"/>
<connect gate="G$1" pin="P4.6/A22" pad="91"/>
<connect gate="G$1" pin="P4.7/A23" pad="92"/>
<connect gate="G$1" pin="P5.1/AN1" pad="28"/>
<connect gate="G$1" pin="P5.10/AN10" pad="39"/>
<connect gate="G$1" pin="P5.11/AN11" pad="40"/>
<connect gate="G$1" pin="P5.12/AN12" pad="41"/>
<connect gate="G$1" pin="P5.13/AN13" pad="42"/>
<connect gate="G$1" pin="P5.14/AN14" pad="43"/>
<connect gate="G$1" pin="P5.15/AN15" pad="44"/>
<connect gate="G$1" pin="P5.2/AN2" pad="29"/>
<connect gate="G$1" pin="P5.3/AN3" pad="30"/>
<connect gate="G$1" pin="P5.4/AN4" pad="31"/>
<connect gate="G$1" pin="P5.5/AN5" pad="32"/>
<connect gate="G$1" pin="P5.6/AN6" pad="33"/>
<connect gate="G$1" pin="P5.7/AN7" pad="34"/>
<connect gate="G$1" pin="P5.8/AN8" pad="35"/>
<connect gate="G$1" pin="P5.9/AN9" pad="36"/>
<connect gate="G$1" pin="P6.0/!CS0" pad="1"/>
<connect gate="G$1" pin="P6.1/!CS1" pad="2"/>
<connect gate="G$1" pin="P6.2/!CS2" pad="3"/>
<connect gate="G$1" pin="P6.3/!CS3" pad="4"/>
<connect gate="G$1" pin="P6.4/!CS4" pad="5"/>
<connect gate="G$1" pin="P6.5/HOLD" pad="6"/>
<connect gate="G$1" pin="P6.6/HLDA" pad="7"/>
<connect gate="G$1" pin="P6.7/BREQ" pad="8"/>
<connect gate="G$1" pin="P7.0/POUT0" pad="19"/>
<connect gate="G$1" pin="P7.1/POUT1" pad="20"/>
<connect gate="G$1" pin="P7.2/POUT2" pad="21"/>
<connect gate="G$1" pin="P7.3/POUT3" pad="22"/>
<connect gate="G$1" pin="P7.4CC28IO" pad="23"/>
<connect gate="G$1" pin="P7.5CC29IO" pad="24"/>
<connect gate="G$1" pin="P7.6CC30IO" pad="25"/>
<connect gate="G$1" pin="P7.7CC31IO" pad="26"/>
<connect gate="G$1" pin="P8.0CC16IO" pad="9"/>
<connect gate="G$1" pin="P8.1CC17IO" pad="10"/>
<connect gate="G$1" pin="P8.2CC18IO" pad="11"/>
<connect gate="G$1" pin="P8.3CC19IO" pad="12"/>
<connect gate="G$1" pin="P8.4CC20IO" pad="13"/>
<connect gate="G$1" pin="P8.5CC21IO" pad="14"/>
<connect gate="G$1" pin="P8.6CC22IO" pad="15"/>
<connect gate="G$1" pin="P8.7CC23IO" pad="16"/>
<connect gate="G$1" pin="VAGND" pad="38"/>
<connect gate="G$1" pin="VAREF" pad="37"/>
<connect gate="G$1" pin="VPP" pad="84"/>
<connect gate="G$1" pin="XTAL1" pad="138"/>
<connect gate="G$1" pin="XTAL2" pad="137"/>
<connect gate="P" pin="VCC@1" pad="17"/>
<connect gate="P" pin="VCC@10" pad="144"/>
<connect gate="P" pin="VCC@2" pad="46"/>
<connect gate="P" pin="VCC@3" pad="56"/>
<connect gate="P" pin="VCC@4" pad="72"/>
<connect gate="P" pin="VCC@5" pad="82"/>
<connect gate="P" pin="VCC@6" pad="93"/>
<connect gate="P" pin="VCC@7" pad="109"/>
<connect gate="P" pin="VCC@8" pad="126"/>
<connect gate="P" pin="VCC@9" pad="136"/>
<connect gate="P" pin="VSS@1" pad="18"/>
<connect gate="P" pin="VSS@10" pad="143"/>
<connect gate="P" pin="VSS@2" pad="45"/>
<connect gate="P" pin="VSS@3" pad="55"/>
<connect gate="P" pin="VSS@4" pad="71"/>
<connect gate="P" pin="VSS@5" pad="83"/>
<connect gate="P" pin="VSS@6" pad="94"/>
<connect gate="P" pin="VSS@7" pad="110"/>
<connect gate="P" pin="VSS@8" pad="127"/>
<connect gate="P" pin="VSS@9" pad="139"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="K">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAF-XC2264" prefix="IC">
<description>&lt;b&gt; 16 Bit Microcontroller &lt;/b&gt;</description>
<gates>
<gate name="G" symbol="SAK-XC226*"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G" pin="/BRKIN_A/P5.10/ADC0_CH10" pad="32"/>
<connect gate="G" pin="/BRKIN_C/P7.1/EXTCLK/TXDC4/CCU62_CTRAPA" pad="8"/>
<connect gate="G" pin="/PORST" pad="97"/>
<connect gate="G" pin="/TESTM" pad="3"/>
<connect gate="G" pin="/TRST" pad="5"/>
<connect gate="G" pin="ESR0" pad="99"/>
<connect gate="G" pin="ESR1/EX0AINB" pad="98"/>
<connect gate="G" pin="P0.0/U1C0_DOUT/CCU61_CC60/U1C0_DX0A/A0" pad="53"/>
<connect gate="G" pin="P0.1/U1C0_DOUT/TXDC0/CCU61_CC61/U1C0_DX0B/U1C0_DX1A/A1" pad="55"/>
<connect gate="G" pin="P0.2/U1C0_SCLKOUT/TXDC0/CCU61_CC62/U1C0_DX1B/A2" pad="58"/>
<connect gate="G" pin="P0.3/U1C0_SELO0/U1C1/SELO1/CCU61_COUT60/U1C0_DX2A/DXDC0B/A3" pad="61"/>
<connect gate="G" pin="P0.4/U1C1_SELO0/U1C0_SELO1/CCU61_COUT61/U1C1_DX2A/RXDC1B/A4" pad="63"/>
<connect gate="G" pin="P0.5/U1C1_SCLKOUT/U1C10_SELO2/CCU61_COUT62/U1C1_DX1A/U1C0_DX1C/A5" pad="68"/>
<connect gate="G" pin="P0.6/U1C1_DOUT/TXDC1/CCU61_COUT63/U1C1_DX0A/CCU61_CTRAPA/U1C1_DX1B/A6" pad="71"/>
<connect gate="G" pin="P0.7/U1C1_DOUT/U1C0_SELO3/U1C1_DX0B/CCU61_CTRAPB/A7" pad="74"/>
<connect gate="G" pin="P1.0/U1C0_MCLKOUT/U1C0_SELO4/EX0BINA/CCU62_CTRAPB/A8" pad="78"/>
<connect gate="G" pin="P1.1/CCU62_COUT62/U1C0_SELO5/U2C1_DOUT/EX1BINA/U2C1_DX0C/A9" pad="81"/>
<connect gate="G" pin="P1.2/CCU62_CC62/U1C0_SELO6/U2C1_SCLKOUT/CCU61_T12HRB/EX2AINA/A2C1_DX0D/U2C1_DX1C/A10" pad="84"/>
<connect gate="G" pin="P1.3/CCU62_COUT63/U1C0_SELO7/U2C0_SELO4/CCU62_T12HRB/EX3AINA/A11" pad="87"/>
<connect gate="G" pin="P1.4/CCU62_COUT61/U1C1_SELO4/U2C0_SELO5/U2C0_DX2B/A12" pad="90"/>
<connect gate="G" pin="P1.5/CCU62_COUT60/U1C1_SELO3/!BRKOUT/U2C0_DX0C/A13" pad="92"/>
<connect gate="G" pin="P1.6/CCU62_CC61/U1C1_SELO2/U2C0_DOUT/U2C0_DX0D/A14" pad="93"/>
<connect gate="G" pin="P1.7/CCU62_CC60/U1C1_MCLKOUT/U2C0_SCLKOUT/U2C0_DX1C/A15" pad="94"/>
<connect gate="G" pin="P10.0/U0C1_DOUT/CCU60_CC60/U0C0_DX0A/U0C1DX0A/AD0" pad="59"/>
<connect gate="G" pin="P10.1/U0C0_DOUT/CCU60_CC61/U0C0_DX0B/U0C0_DX1A/AD1" pad="60"/>
<connect gate="G" pin="P10.10/TDI_B/U0C1_DX1A/U0C0_DX2C/CCU60_COUT63/U0C0_SELO0/AD10" pad="82"/>
<connect gate="G" pin="P10.11/U1C0_SCLKOUT/!BRKOUT/U1C0_DX1D/RXDC2B/TMS_B/AD11" pad="83"/>
<connect gate="G" pin="P10.12/U1C0_DOUT/TXDC2/TDO/U1C0_DX0C/U1C0_DX1E/AD12" pad="85"/>
<connect gate="G" pin="P10.13/U1C0_DOUT/TXDC3/U1C0_SELO3/U1C0_DX0D/!WRL/!WR" pad="86"/>
<connect gate="G" pin="P10.14/U1C0_SELO1/U0C1_DX0C/RXDC3C/!RD" pad="89"/>
<connect gate="G" pin="P10.15/U1C0_SELO2/U0C1_DOUT/U1C0_DOUT/U0C1_DX1C/ALE" pad="91"/>
<connect gate="G" pin="P10.2/U0C0_SCLKOUT/U0C0_DX1B/AD2" pad="62"/>
<connect gate="G" pin="P10.3/CCU60_COUT60/U0C0_DX2A/U0C1_DX2A/AD3" pad="67"/>
<connect gate="G" pin="P10.4/U0C0_SELO3/CCU60_COUT61/U0C0_DX2B/U0C1_DX2B/AD4" pad="69"/>
<connect gate="G" pin="P10.5/U0C1_SCLKOUT/CCU60_COUT62/U0C1_DX1B/AD5" pad="70"/>
<connect gate="G" pin="P10.6/U0C0_DOUT/TXDC4/U1C0_SELO0/U0C0_DX0C/U1C0_DX2D/CCU60_CTRAPA/AD6" pad="72"/>
<connect gate="G" pin="P10.7/U0C1_DOUT/CCU60_COUT63/U0C1_DX0B/CCU60_CCPOS0A/DXD4C/AD7" pad="73"/>
<connect gate="G" pin="P10.8/!BRKIN_B/U0C0_DX1C/CCU60_CCPOS1A/U0C1_SELO0/U0C0_MCLKOUT/AD8" pad="79"/>
<connect gate="G" pin="P10.9/U0C0_SELO4/U0C1_MCLKOUT/CCU60_CCPOS2A/TCK_B/AD9" pad="80"/>
<connect gate="G" pin="P15.0/ADC1_CH0" pad="15"/>
<connect gate="G" pin="P15.2/ADC1_CH2/T5IN" pad="16"/>
<connect gate="G" pin="P15.4/ADC1_CH4/T6IN" pad="17"/>
<connect gate="G" pin="P15.5/ADC1_CH5/T6EUD" pad="18"/>
<connect gate="G" pin="P15.6/ADC1_CH6" pad="19"/>
<connect gate="G" pin="P2.0/CCU63_CC60/AD13/RXDC0C" pad="39"/>
<connect gate="G" pin="P2.1/TXDC0/CCU63_CC61/AD14/EX0AINA" pad="40"/>
<connect gate="G" pin="P2.10/U0C1_DOUT/U0C0_SELO3/CC2_7/A23/U0C1_DX0E/CAPIN" pad="66"/>
<connect gate="G" pin="P2.11/U0C0_SELO2/U0C1_SELO2/!BHE/!WRH" pad="37"/>
<connect gate="G" pin="P2.12/U0C0_SELO4/U0C1_SELO3/READY" pad="36"/>
<connect gate="G" pin="P2.2/TXDC1/CCU63_CC62/AD15/EX1AINA" pad="41"/>
<connect gate="G" pin="P2.3/U0C0_DOUT/CCU63_COUT63/CC2_0/A16/U0C0_DX0E/U0C1_DX0D/RXDC0A" pad="43"/>
<connect gate="G" pin="P2.4/U0C1_DOUT/TXDC0/CC2_1/A17/U0C0_DX0F/RXDC1A" pad="45"/>
<connect gate="G" pin="P2.5/U0C0_SCLKOUT/TXDC0/CC2_2/A18/A0C0_DX1D" pad="46"/>
<connect gate="G" pin="P2.6/U0C0_SELO0/U0C1_SELO1/CC2_3/A19/U0C0_DX2D/RXDC0D" pad="48"/>
<connect gate="G" pin="P2.7/U0C1_SELO0/U0C0_SELO1/CC2_4/A20/U0C1_DX2C/RXDC1C" pad="54"/>
<connect gate="G" pin="P2.8/U0C1_SCLKOUT/EXTCLK/CC2_5/A21/U0C1_DX1D" pad="56"/>
<connect gate="G" pin="P4.0/CC2_8/!CS0" pad="42"/>
<connect gate="G" pin="P4.1/TXDC2/CC2_9/!CS1" pad="44"/>
<connect gate="G" pin="P4.2/TXDC2/CC2_10/T2IN/!CS2" pad="47"/>
<connect gate="G" pin="P4.3/CC2_11/RXDC2A/T2EUD/!CS3" pad="49"/>
<connect gate="G" pin="P5.0/ADC0_CH0" pad="22"/>
<connect gate="G" pin="P5.11/ADC0_CH11" pad="33"/>
<connect gate="G" pin="P5.13/ADC0_CH10/EX0BINB" pad="34"/>
<connect gate="G" pin="P5.15/ADC0_CH15" pad="35"/>
<connect gate="G" pin="P5.3/ADC0_CH3/T3IN" pad="24"/>
<connect gate="G" pin="P5.5/ADC0_CH5/CCU60_T12HRB" pad="29"/>
<connect gate="G" pin="P5.8/ADC0_CH8/CCU6X_T12HRC/CCU6X_T13HRC" pad="30"/>
<connect gate="G" pin="P5.9/ADC0_CH9/CC2_T7IN" pad="31"/>
<connect gate="G" pin="P6.0/EMUX0/U1C1_DOUT/!BRKOUT/ADCX_REQGTYC/U1C1_DX0E" pad="11"/>
<connect gate="G" pin="P6.1/EMUX1/T3OUT/U1C1_DOUT/ADCX_REQTRYC" pad="12"/>
<connect gate="G" pin="P6.2/EMUX2/T6OUT/U1C1_SCLK/U1C1_DXC1" pad="13"/>
<connect gate="G" pin="TCK_A/P2.9/U0C1_DOUT/TXDC1/CC2_6/A22/DIRIN/" pad="57"/>
<connect gate="G" pin="TCK_C/P7.4/EMUX2/U0C1DOUT/U0C1_SCLK/CCU62_CCPOS2A/U0C0_DX0D/U1C1_DX1E" pad="9"/>
<connect gate="G" pin="TDI_A/P5.2/ADC0_CH2" pad="23"/>
<connect gate="G" pin="TDI_C/P7,2/EMUX0/TXDC4/CCU62_CCPOS0A" pad="4"/>
<connect gate="G" pin="TDO/P7.0/T3OUT/T6OUT/RXDC4B" pad="6"/>
<connect gate="G" pin="TMS_A/P5.4/ADC0_CH4/CCU63_T12HRB/T3EUD" pad="28"/>
<connect gate="G" pin="TMS_C/P7.3/EMUX1/U01_DOUT/U0C0_DOUT/CCU62_CCPOS1A/U0C1DX0F" pad="7"/>
<connect gate="G" pin="TREF" pad="65"/>
<connect gate="G" pin="VAGND" pad="21"/>
<connect gate="G" pin="VAREF" pad="20"/>
<connect gate="G" pin="VDD@1" pad="38"/>
<connect gate="G" pin="VDD@2" pad="88"/>
<connect gate="G" pin="VDDI@1" pad="64"/>
<connect gate="G" pin="VDDIM@0" pad="10"/>
<connect gate="G" pin="VDDPA@0" pad="14"/>
<connect gate="G" pin="VDDPB@0" pad="2"/>
<connect gate="G" pin="VDDPB@1" pad="100"/>
<connect gate="G" pin="VDDPB@2" pad="25"/>
<connect gate="G" pin="VDDPB@3" pad="27"/>
<connect gate="G" pin="VDDPB@4" pad="50"/>
<connect gate="G" pin="VDDPB@5" pad="52"/>
<connect gate="G" pin="VDDPB@6" pad="75"/>
<connect gate="G" pin="VDDPB@7" pad="77"/>
<connect gate="G" pin="VSS@0" pad="1"/>
<connect gate="G" pin="VSS@1" pad="26"/>
<connect gate="G" pin="VSS@2" pad="51"/>
<connect gate="G" pin="VSS@4" pad="76"/>
<connect gate="G" pin="XTAL1" pad="96"/>
<connect gate="G" pin="XTAL2" pad="95"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAK-TC1100*" prefix="IC">
<description>&lt;b&gt;32-bit Consumer Class TriCore&lt;/b&gt; Single-Chip Microcontroller&lt;p&gt;
Source: http://www.infineon.com/cmc_upload/documents/010/9915/TC1100_umsu_v10.pdf</description>
<gates>
<gate name="-C" symbol="TC1100"/>
<gate name="-P0" symbol="PORT16"/>
<gate name="-P1" symbol="PORT16"/>
<gate name="-P2" symbol="PORT16"/>
<gate name="-P3" symbol="PORT16"/>
<gate name="-P4" symbol="PORT8"/>
<gate name="-AD" symbol="AD31"/>
<gate name="-A" symbol="A23"/>
<gate name="-JTAG" symbol="JTAG"/>
<gate name="-VSS1" symbol="VSS"/>
<gate name="-VSS2" symbol="VSS"/>
<gate name="-VSS3" symbol="VSS"/>
<gate name="-VSS4" symbol="VSS"/>
<gate name="-VSS5" symbol="VSS"/>
<gate name="-VSS6" symbol="VSS"/>
<gate name="-VSS7" symbol="VSS"/>
<gate name="-VSS8" symbol="VSS"/>
<gate name="-VSS9" symbol="VSS"/>
<gate name="-VSS10" symbol="VSS"/>
<gate name="-VSS11" symbol="VSS"/>
<gate name="-VSS12" symbol="VSS"/>
<gate name="-VSS13" symbol="VSS"/>
<gate name="-VSS14" symbol="VSS"/>
<gate name="-VSS15" symbol="VSS"/>
<gate name="-VSS16" symbol="VSS"/>
<gate name="-VDD1" symbol="VDD"/>
<gate name="-VDD2" symbol="VDD"/>
<gate name="-VDD3" symbol="VDD"/>
<gate name="-VDD4" symbol="VDD"/>
<gate name="-VDD5" symbol="VDD"/>
<gate name="-VDD6" symbol="VDD"/>
<gate name="-VDD7" symbol="VDD"/>
<gate name="-VDD8" symbol="VDD"/>
<gate name="-VDD9" symbol="VDD"/>
<gate name="-VDDP1" symbol="VDDP"/>
<gate name="-VDDP2" symbol="VDDP"/>
<gate name="-VDDP3" symbol="VDDP"/>
<gate name="-VDDP4" symbol="VDDP"/>
<gate name="-VDDP5" symbol="VDDP"/>
<gate name="-VDDP6" symbol="VDDP"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="-A" pin="A0" pad="K1"/>
<connect gate="-A" pin="A1" pad="L1"/>
<connect gate="-A" pin="A10" pad="J3"/>
<connect gate="-A" pin="A11" pad="K3"/>
<connect gate="-A" pin="A12" pad="L3"/>
<connect gate="-A" pin="A13" pad="M3"/>
<connect gate="-A" pin="A14" pad="K4"/>
<connect gate="-A" pin="A15" pad="A8"/>
<connect gate="-A" pin="A16" pad="A9"/>
<connect gate="-A" pin="A17" pad="A10"/>
<connect gate="-A" pin="A18" pad="B10"/>
<connect gate="-A" pin="A19" pad="C10"/>
<connect gate="-A" pin="A2" pad="M1"/>
<connect gate="-A" pin="A20" pad="D10"/>
<connect gate="-A" pin="A21" pad="T4"/>
<connect gate="-A" pin="A22" pad="R4"/>
<connect gate="-A" pin="A23" pad="P4"/>
<connect gate="-A" pin="A3" pad="N1"/>
<connect gate="-A" pin="A4" pad="P1"/>
<connect gate="-A" pin="A5" pad="J2"/>
<connect gate="-A" pin="A6" pad="K2"/>
<connect gate="-A" pin="A7" pad="L2"/>
<connect gate="-A" pin="A8" pad="M2"/>
<connect gate="-A" pin="A9" pad="N2"/>
<connect gate="-AD" pin="AD0" pad="C8"/>
<connect gate="-AD" pin="AD1" pad="C7"/>
<connect gate="-AD" pin="AD10" pad="F1"/>
<connect gate="-AD" pin="AD11" pad="E3"/>
<connect gate="-AD" pin="AD12" pad="F3"/>
<connect gate="-AD" pin="AD13" pad="G1"/>
<connect gate="-AD" pin="AD14" pad="H2"/>
<connect gate="-AD" pin="AD15" pad="G3"/>
<connect gate="-AD" pin="AD16" pad="D7"/>
<connect gate="-AD" pin="AD17" pad="B5"/>
<connect gate="-AD" pin="AD18" pad="A4"/>
<connect gate="-AD" pin="AD19" pad="B4"/>
<connect gate="-AD" pin="AD2" pad="B6"/>
<connect gate="-AD" pin="AD20" pad="C4"/>
<connect gate="-AD" pin="AD21" pad="B3"/>
<connect gate="-AD" pin="AD22" pad="B2"/>
<connect gate="-AD" pin="AD23" pad="B1"/>
<connect gate="-AD" pin="AD24" pad="C1"/>
<connect gate="-AD" pin="AD25" pad="D3"/>
<connect gate="-AD" pin="AD26" pad="E2"/>
<connect gate="-AD" pin="AD27" pad="F2"/>
<connect gate="-AD" pin="AD28" pad="F4"/>
<connect gate="-AD" pin="AD29" pad="G4"/>
<connect gate="-AD" pin="AD3" pad="C6"/>
<connect gate="-AD" pin="AD30" pad="H3"/>
<connect gate="-AD" pin="AD31" pad="G2"/>
<connect gate="-AD" pin="AD4" pad="C5"/>
<connect gate="-AD" pin="AD5" pad="A3"/>
<connect gate="-AD" pin="AD6" pad="A2"/>
<connect gate="-AD" pin="AD7" pad="C3"/>
<connect gate="-AD" pin="AD8" pad="C2"/>
<connect gate="-AD" pin="AD9" pad="D2"/>
<connect gate="-C" pin="!ADV" pad="B11"/>
<connect gate="-C" pin="!BAA" pad="A11"/>
<connect gate="-C" pin="!BC0" pad="A5"/>
<connect gate="-C" pin="!BC1" pad="A6"/>
<connect gate="-C" pin="!BC2" pad="B7"/>
<connect gate="-C" pin="!BC3" pad="A7"/>
<connect gate="-C" pin="!BRKIN" pad="T5"/>
<connect gate="-C" pin="!CAS" pad="D5"/>
<connect gate="-C" pin="!CS0" pad="D9"/>
<connect gate="-C" pin="!CS1" pad="D8"/>
<connect gate="-C" pin="!CS2" pad="C9"/>
<connect gate="-C" pin="!CS3" pad="B8"/>
<connect gate="-C" pin="!CSCOMB" pad="N3"/>
<connect gate="-C" pin="!HDRST" pad="N5"/>
<connect gate="-C" pin="!MR_W" pad="P3"/>
<connect gate="-C" pin="!NMI" pad="T7"/>
<connect gate="-C" pin="!PORST" pad="R5"/>
<connect gate="-C" pin="!RAS" pad="D6"/>
<connect gate="-C" pin="!RD" pad="P2"/>
<connect gate="-C" pin="!RD_WR" pad="T3"/>
<connect gate="-C" pin="!TRCLK" pad="T8"/>
<connect gate="-C" pin="!WAIT" pad="B9"/>
<connect gate="-C" pin="ALE" pad="R3"/>
<connect gate="-C" pin="BFCLKI" pad="D1"/>
<connect gate="-C" pin="BFCLKO" pad="E1"/>
<connect gate="-C" pin="CKE" pad="L4"/>
<connect gate="-C" pin="HWCFG0" pad="M14"/>
<connect gate="-C" pin="HWCFG1" pad="L14"/>
<connect gate="-C" pin="HWCFG2" pad="T6"/>
<connect gate="-C" pin="NC@1" pad="R1"/>
<connect gate="-C" pin="NC@2" pad="T14"/>
<connect gate="-C" pin="NC@3" pad="T15"/>
<connect gate="-C" pin="RESERVED@1" pad="A1"/>
<connect gate="-C" pin="RESERVED@2" pad="A16"/>
<connect gate="-C" pin="RESERVED@3" pad="T1"/>
<connect gate="-C" pin="RESERVED@4" pad="T16"/>
<connect gate="-C" pin="SDCLKI" pad="J1"/>
<connect gate="-C" pin="SDCLKO" pad="H1"/>
<connect gate="-C" pin="VDDOSC" pad="L16"/>
<connect gate="-C" pin="VDDOSC3" pad="P16"/>
<connect gate="-C" pin="VSSOSC" pad="L15"/>
<connect gate="-C" pin="VSSOSC3" pad="R16"/>
<connect gate="-C" pin="XTAL1" pad="M16"/>
<connect gate="-C" pin="XTAL2" pad="N16"/>
<connect gate="-JTAG" pin="!TRST" pad="T11"/>
<connect gate="-JTAG" pin="TCK" pad="T12"/>
<connect gate="-JTAG" pin="TDI" pad="T13"/>
<connect gate="-JTAG" pin="TDO" pad="T10"/>
<connect gate="-JTAG" pin="TMS" pad="T9"/>
<connect gate="-P0" pin="0" pad="N11"/>
<connect gate="-P0" pin="1" pad="P15"/>
<connect gate="-P0" pin="10" pad="R14"/>
<connect gate="-P0" pin="11" pad="N9"/>
<connect gate="-P0" pin="12" pad="P9"/>
<connect gate="-P0" pin="13" pad="P8"/>
<connect gate="-P0" pin="14" pad="N8"/>
<connect gate="-P0" pin="15" pad="P7"/>
<connect gate="-P0" pin="2" pad="P10"/>
<connect gate="-P0" pin="3" pad="M15"/>
<connect gate="-P0" pin="4" pad="R11"/>
<connect gate="-P0" pin="5" pad="R12"/>
<connect gate="-P0" pin="6" pad="R10"/>
<connect gate="-P0" pin="7" pad="N10"/>
<connect gate="-P0" pin="8" pad="R13"/>
<connect gate="-P0" pin="9" pad="R15"/>
<connect gate="-P1" pin="0" pad="D11"/>
<connect gate="-P1" pin="1" pad="C12"/>
<connect gate="-P1" pin="10" pad="B14"/>
<connect gate="-P1" pin="11" pad="C14"/>
<connect gate="-P1" pin="12" pad="F13"/>
<connect gate="-P1" pin="13" pad="E14"/>
<connect gate="-P1" pin="14" pad="D14"/>
<connect gate="-P1" pin="15" pad="F14"/>
<connect gate="-P1" pin="2" pad="D12"/>
<connect gate="-P1" pin="3" pad="B12"/>
<connect gate="-P1" pin="4" pad="C11"/>
<connect gate="-P1" pin="5" pad="C13"/>
<connect gate="-P1" pin="6" pad="A12"/>
<connect gate="-P1" pin="7" pad="B13"/>
<connect gate="-P1" pin="8" pad="A13"/>
<connect gate="-P1" pin="9" pad="A14"/>
<connect gate="-P2" pin="0" pad="P12"/>
<connect gate="-P2" pin="1" pad="P11"/>
<connect gate="-P2" pin="10" pad="L13"/>
<connect gate="-P2" pin="11" pad="G16"/>
<connect gate="-P2" pin="12" pad="K15"/>
<connect gate="-P2" pin="13" pad="K14"/>
<connect gate="-P2" pin="14" pad="F16"/>
<connect gate="-P2" pin="15" pad="E16"/>
<connect gate="-P2" pin="2" pad="P13"/>
<connect gate="-P2" pin="3" pad="P14"/>
<connect gate="-P2" pin="4" pad="N15"/>
<connect gate="-P2" pin="5" pad="N14"/>
<connect gate="-P2" pin="6" pad="N12"/>
<connect gate="-P2" pin="7" pad="K16"/>
<connect gate="-P2" pin="8" pad="J16"/>
<connect gate="-P2" pin="9" pad="H16"/>
<connect gate="-P3" pin="0" pad="A15"/>
<connect gate="-P3" pin="1" pad="B15"/>
<connect gate="-P3" pin="10" pad="B16"/>
<connect gate="-P3" pin="11" pad="C16"/>
<connect gate="-P3" pin="12" pad="D16"/>
<connect gate="-P3" pin="13" pad="K13"/>
<connect gate="-P3" pin="14" pad="J14"/>
<connect gate="-P3" pin="15" pad="J15"/>
<connect gate="-P3" pin="2" pad="D15"/>
<connect gate="-P3" pin="3" pad="E15"/>
<connect gate="-P3" pin="4" pad="G14"/>
<connect gate="-P3" pin="5" pad="G15"/>
<connect gate="-P3" pin="6" pad="F15"/>
<connect gate="-P3" pin="7" pad="H14"/>
<connect gate="-P3" pin="8" pad="C15"/>
<connect gate="-P3" pin="9" pad="H15"/>
<connect gate="-P4" pin="0" pad="R8"/>
<connect gate="-P4" pin="1" pad="R9"/>
<connect gate="-P4" pin="2" pad="N7"/>
<connect gate="-P4" pin="3" pad="N6"/>
<connect gate="-P4" pin="4" pad="P6"/>
<connect gate="-P4" pin="5" pad="R7"/>
<connect gate="-P4" pin="6" pad="R6"/>
<connect gate="-P4" pin="7" pad="P5"/>
<connect gate="-VDD1" pin="VDD" pad="G7"/>
<connect gate="-VDD2" pin="VDD" pad="G8"/>
<connect gate="-VDD3" pin="VDD" pad="G9"/>
<connect gate="-VDD4" pin="VDD" pad="G10"/>
<connect gate="-VDD5" pin="VDD" pad="G13"/>
<connect gate="-VDD6" pin="VDD" pad="K7"/>
<connect gate="-VDD7" pin="VDD" pad="K8"/>
<connect gate="-VDD8" pin="VDD" pad="K9"/>
<connect gate="-VDD9" pin="VDD" pad="K10"/>
<connect gate="-VDDP1" pin="VDDP" pad="D4"/>
<connect gate="-VDDP2" pin="VDDP" pad="D13"/>
<connect gate="-VDDP3" pin="VDDP" pad="H4"/>
<connect gate="-VDDP4" pin="VDDP" pad="J13"/>
<connect gate="-VDDP5" pin="VDDP" pad="M4"/>
<connect gate="-VDDP6" pin="VDDP" pad="N13"/>
<connect gate="-VSS1" pin="VSS" pad="E4"/>
<connect gate="-VSS10" pin="VSS" pad="J8"/>
<connect gate="-VSS11" pin="VSS" pad="J9"/>
<connect gate="-VSS12" pin="VSS" pad="J10"/>
<connect gate="-VSS13" pin="VSS" pad="M13"/>
<connect gate="-VSS14" pin="VSS" pad="N4"/>
<connect gate="-VSS15" pin="VSS" pad="R2"/>
<connect gate="-VSS16" pin="VSS" pad="T2"/>
<connect gate="-VSS2" pin="VSS" pad="E13"/>
<connect gate="-VSS3" pin="VSS" pad="H7"/>
<connect gate="-VSS4" pin="VSS" pad="H8"/>
<connect gate="-VSS5" pin="VSS" pad="H9"/>
<connect gate="-VSS6" pin="VSS" pad="H10"/>
<connect gate="-VSS7" pin="VSS" pad="H13"/>
<connect gate="-VSS8" pin="VSS" pad="J4"/>
<connect gate="-VSS9" pin="VSS" pad="J7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAK-TC1130*" prefix="IC">
<description>&lt;b&gt; 32-Bit Industrial &amp;Communication Controller&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. TC1130_DS_v031.pdf</description>
<gates>
<gate name="G" symbol="TC1130"/>
<gate name="PWR" symbol="PWR_TC1130"/>
<gate name="P0" symbol="PORT16"/>
<gate name="P1" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="P3" symbol="PORT16"/>
<gate name="RES" symbol="NC4"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="G" pin="/ADV" pad="B11"/>
<connect gate="G" pin="/BAA" pad="A11"/>
<connect gate="G" pin="/BRKIN" pad="T5"/>
<connect gate="G" pin="/CAS" pad="D5"/>
<connect gate="G" pin="/CSCOMB" pad="N3"/>
<connect gate="G" pin="/HDRST" pad="N5"/>
<connect gate="G" pin="/MR_W" pad="P3"/>
<connect gate="G" pin="/PORST" pad="R5"/>
<connect gate="G" pin="/RAS" pad="D6"/>
<connect gate="G" pin="/RD" pad="P2"/>
<connect gate="G" pin="/WAIT" pad="B9"/>
<connect gate="G" pin="/WR" pad="T3"/>
<connect gate="G" pin="A0" pad="K1"/>
<connect gate="G" pin="A1" pad="L1"/>
<connect gate="G" pin="A10" pad="J3"/>
<connect gate="G" pin="A11" pad="K3"/>
<connect gate="G" pin="A12" pad="L3"/>
<connect gate="G" pin="A13" pad="M3"/>
<connect gate="G" pin="A14" pad="K4"/>
<connect gate="G" pin="A15" pad="A8"/>
<connect gate="G" pin="A16" pad="A9"/>
<connect gate="G" pin="A17" pad="A10"/>
<connect gate="G" pin="A18" pad="B10"/>
<connect gate="G" pin="A19" pad="C10"/>
<connect gate="G" pin="A2" pad="M1"/>
<connect gate="G" pin="A20" pad="D10"/>
<connect gate="G" pin="A21" pad="T4"/>
<connect gate="G" pin="A22" pad="R4"/>
<connect gate="G" pin="A23" pad="P4"/>
<connect gate="G" pin="A3" pad="N1"/>
<connect gate="G" pin="A4" pad="P1"/>
<connect gate="G" pin="A5" pad="J2"/>
<connect gate="G" pin="A6" pad="K2"/>
<connect gate="G" pin="A7" pad="L2"/>
<connect gate="G" pin="A8" pad="M2"/>
<connect gate="G" pin="A9" pad="N2"/>
<connect gate="G" pin="AD0" pad="C8"/>
<connect gate="G" pin="AD1" pad="C7"/>
<connect gate="G" pin="AD10" pad="F1"/>
<connect gate="G" pin="AD11" pad="E3"/>
<connect gate="G" pin="AD12" pad="F3"/>
<connect gate="G" pin="AD13" pad="G1"/>
<connect gate="G" pin="AD14" pad="H2"/>
<connect gate="G" pin="AD15" pad="G3"/>
<connect gate="G" pin="AD16" pad="D7"/>
<connect gate="G" pin="AD17" pad="B5"/>
<connect gate="G" pin="AD18" pad="A4"/>
<connect gate="G" pin="AD19" pad="B4"/>
<connect gate="G" pin="AD2" pad="B6"/>
<connect gate="G" pin="AD20" pad="C4"/>
<connect gate="G" pin="AD21" pad="B3"/>
<connect gate="G" pin="AD22" pad="B2"/>
<connect gate="G" pin="AD23" pad="B1"/>
<connect gate="G" pin="AD24" pad="C1"/>
<connect gate="G" pin="AD25" pad="D3"/>
<connect gate="G" pin="AD26" pad="E2"/>
<connect gate="G" pin="AD27" pad="F2"/>
<connect gate="G" pin="AD28" pad="F4"/>
<connect gate="G" pin="AD29" pad="G4"/>
<connect gate="G" pin="AD3" pad="C6"/>
<connect gate="G" pin="AD30" pad="H3"/>
<connect gate="G" pin="AD31" pad="G2"/>
<connect gate="G" pin="AD4" pad="C5"/>
<connect gate="G" pin="AD5" pad="A3"/>
<connect gate="G" pin="AD6" pad="A2"/>
<connect gate="G" pin="AD7" pad="C3"/>
<connect gate="G" pin="AD8" pad="C2"/>
<connect gate="G" pin="AD9" pad="D2"/>
<connect gate="G" pin="ALE" pad="R3"/>
<connect gate="G" pin="BC0" pad="A5"/>
<connect gate="G" pin="BC1" pad="A6"/>
<connect gate="G" pin="BC2" pad="B7"/>
<connect gate="G" pin="BC3" pad="A7"/>
<connect gate="G" pin="BFCLKI" pad="D1"/>
<connect gate="G" pin="BFCLKO" pad="E1"/>
<connect gate="G" pin="CKE" pad="L4"/>
<connect gate="G" pin="CS0" pad="D9"/>
<connect gate="G" pin="CS1" pad="D8"/>
<connect gate="G" pin="CS2" pad="C9"/>
<connect gate="G" pin="CS3" pad="B8"/>
<connect gate="G" pin="D+" pad="T14"/>
<connect gate="G" pin="D-" pad="T15"/>
<connect gate="G" pin="HWCFG0" pad="M14"/>
<connect gate="G" pin="HWCFG1" pad="L14"/>
<connect gate="G" pin="HWCFG2" pad="T6"/>
<connect gate="G" pin="MI_MDIO" pad="R1"/>
<connect gate="G" pin="MI_RXCLK" pad="R2"/>
<connect gate="G" pin="MI_TXCLK" pad="T2"/>
<connect gate="G" pin="NMI" pad="T7"/>
<connect gate="G" pin="P4.0" pad="R8"/>
<connect gate="G" pin="P4.1" pad="R9"/>
<connect gate="G" pin="P4.2" pad="N7"/>
<connect gate="G" pin="P4.3" pad="N6"/>
<connect gate="G" pin="P4.4" pad="P6"/>
<connect gate="G" pin="P4.5" pad="R7"/>
<connect gate="G" pin="P4.6" pad="R6"/>
<connect gate="G" pin="P4.7" pad="P5"/>
<connect gate="G" pin="SDCLKI" pad="J1"/>
<connect gate="G" pin="SDCLKO" pad="H1"/>
<connect gate="G" pin="TCK" pad="T12"/>
<connect gate="G" pin="TDI" pad="T13"/>
<connect gate="G" pin="TDO" pad="T10"/>
<connect gate="G" pin="TMS" pad="T9"/>
<connect gate="G" pin="TRCLK" pad="T8"/>
<connect gate="G" pin="TRST" pad="T11"/>
<connect gate="G" pin="VDDOSC" pad="L16"/>
<connect gate="G" pin="VDDOSC3" pad="P16"/>
<connect gate="G" pin="VSSOSC" pad="N4"/>
<connect gate="G" pin="VSSOSC3" pad="R16"/>
<connect gate="G" pin="XTAL1" pad="M16"/>
<connect gate="G" pin="XTAL2" pad="N16"/>
<connect gate="P0" pin="0" pad="N11"/>
<connect gate="P0" pin="1" pad="P15"/>
<connect gate="P0" pin="10" pad="R14"/>
<connect gate="P0" pin="11" pad="N9"/>
<connect gate="P0" pin="12" pad="P9"/>
<connect gate="P0" pin="13" pad="P8"/>
<connect gate="P0" pin="14" pad="N8"/>
<connect gate="P0" pin="15" pad="P7"/>
<connect gate="P0" pin="2" pad="P10"/>
<connect gate="P0" pin="3" pad="M15"/>
<connect gate="P0" pin="4" pad="R11"/>
<connect gate="P0" pin="5" pad="R12"/>
<connect gate="P0" pin="6" pad="R10"/>
<connect gate="P0" pin="7" pad="N10"/>
<connect gate="P0" pin="8" pad="R13"/>
<connect gate="P0" pin="9" pad="R15"/>
<connect gate="P1" pin="0" pad="D11"/>
<connect gate="P1" pin="1" pad="C12"/>
<connect gate="P1" pin="10" pad="B14"/>
<connect gate="P1" pin="11" pad="C14"/>
<connect gate="P1" pin="12" pad="F13"/>
<connect gate="P1" pin="13" pad="E14"/>
<connect gate="P1" pin="14" pad="D14"/>
<connect gate="P1" pin="15" pad="F14"/>
<connect gate="P1" pin="2" pad="D12"/>
<connect gate="P1" pin="3" pad="B12"/>
<connect gate="P1" pin="4" pad="C11"/>
<connect gate="P1" pin="5" pad="C13"/>
<connect gate="P1" pin="6" pad="A12"/>
<connect gate="P1" pin="7" pad="B13"/>
<connect gate="P1" pin="8" pad="A13"/>
<connect gate="P1" pin="9" pad="A14"/>
<connect gate="P2" pin="0" pad="P12"/>
<connect gate="P2" pin="1" pad="P11"/>
<connect gate="P2" pin="10" pad="L13"/>
<connect gate="P2" pin="11" pad="G16"/>
<connect gate="P2" pin="12" pad="K15"/>
<connect gate="P2" pin="13" pad="K14"/>
<connect gate="P2" pin="14" pad="F16"/>
<connect gate="P2" pin="15" pad="E16"/>
<connect gate="P2" pin="2" pad="P13"/>
<connect gate="P2" pin="3" pad="P14"/>
<connect gate="P2" pin="4" pad="N15"/>
<connect gate="P2" pin="5" pad="N14"/>
<connect gate="P2" pin="6" pad="N12"/>
<connect gate="P2" pin="7" pad="K16"/>
<connect gate="P2" pin="8" pad="J16"/>
<connect gate="P2" pin="9" pad="H16"/>
<connect gate="P3" pin="0" pad="A15"/>
<connect gate="P3" pin="1" pad="B15"/>
<connect gate="P3" pin="10" pad="B16"/>
<connect gate="P3" pin="11" pad="C16"/>
<connect gate="P3" pin="12" pad="D16"/>
<connect gate="P3" pin="13" pad="K13"/>
<connect gate="P3" pin="14" pad="J14"/>
<connect gate="P3" pin="15" pad="J15"/>
<connect gate="P3" pin="2" pad="D15"/>
<connect gate="P3" pin="3" pad="E15"/>
<connect gate="P3" pin="4" pad="G14"/>
<connect gate="P3" pin="5" pad="G15"/>
<connect gate="P3" pin="6" pad="F15"/>
<connect gate="P3" pin="7" pad="H14"/>
<connect gate="P3" pin="8" pad="C15"/>
<connect gate="P3" pin="9" pad="H15"/>
<connect gate="PWR" pin="VDD@0" pad="G7"/>
<connect gate="PWR" pin="VDD@1" pad="G8"/>
<connect gate="PWR" pin="VDD@2" pad="G9"/>
<connect gate="PWR" pin="VDD@3" pad="G10"/>
<connect gate="PWR" pin="VDD@4" pad="G13"/>
<connect gate="PWR" pin="VDD@5" pad="K7"/>
<connect gate="PWR" pin="VDD@6" pad="K8"/>
<connect gate="PWR" pin="VDD@7" pad="K9"/>
<connect gate="PWR" pin="VDD@8" pad="K10"/>
<connect gate="PWR" pin="VDDP@0" pad="D4"/>
<connect gate="PWR" pin="VDDP@1" pad="D13"/>
<connect gate="PWR" pin="VDDP@2" pad="H4"/>
<connect gate="PWR" pin="VDDP@3" pad="J13"/>
<connect gate="PWR" pin="VDDP@4" pad="M4"/>
<connect gate="PWR" pin="VDDP@5" pad="N13"/>
<connect gate="PWR" pin="VSS@0" pad="E4"/>
<connect gate="PWR" pin="VSS@1" pad="E13"/>
<connect gate="PWR" pin="VSS@10" pad="J9"/>
<connect gate="PWR" pin="VSS@11" pad="J10"/>
<connect gate="PWR" pin="VSS@12" pad="L15"/>
<connect gate="PWR" pin="VSS@13" pad="M13"/>
<connect gate="PWR" pin="VSS@2" pad="H7"/>
<connect gate="PWR" pin="VSS@3" pad="H8"/>
<connect gate="PWR" pin="VSS@4" pad="H9"/>
<connect gate="PWR" pin="VSS@5" pad="H10"/>
<connect gate="PWR" pin="VSS@6" pad="H13"/>
<connect gate="PWR" pin="VSS@7" pad="J4"/>
<connect gate="PWR" pin="VSS@8" pad="J7"/>
<connect gate="PWR" pin="VSS@9" pad="J8"/>
<connect gate="RES" pin="RESERVED@0" pad="A1"/>
<connect gate="RES" pin="RESERVED@1" pad="A16"/>
<connect gate="RES" pin="RESERVED@2" pad="T1"/>
<connect gate="RES" pin="RESERVED@3" pad="T16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAK-TC1762*" prefix="IC">
<description>Infineon TriCore NG (Next Generation) 32bit Microcontroller/DSP</description>
<gates>
<gate name="G" symbol="TC1762"/>
<gate name="PWR" symbol="PWR_TC1762"/>
</gates>
<devices>
<device name="" package="P-LQFP-176-2">
<connects>
<connect gate="G" pin="/BRKIN" pad="117"/>
<connect gate="G" pin="/BRKOUT" pad="116"/>
<connect gate="G" pin="/HDRST" pad="122"/>
<connect gate="G" pin="/NMI" pad="120"/>
<connect gate="G" pin="/PORST" pad="121"/>
<connect gate="G" pin="/TEST_MODE" pad="118"/>
<connect gate="G" pin="/TRST" pad="114"/>
<connect gate="G" pin="AN0" pad="67"/>
<connect gate="G" pin="AN1" pad="66"/>
<connect gate="G" pin="AN10" pad="58"/>
<connect gate="G" pin="AN11" pad="57"/>
<connect gate="G" pin="AN12" pad="56"/>
<connect gate="G" pin="AN13" pad="55"/>
<connect gate="G" pin="AN14" pad="50"/>
<connect gate="G" pin="AN15" pad="49"/>
<connect gate="G" pin="AN16" pad="48"/>
<connect gate="G" pin="AN17" pad="47"/>
<connect gate="G" pin="AN18" pad="46"/>
<connect gate="G" pin="AN19" pad="45"/>
<connect gate="G" pin="AN2" pad="65"/>
<connect gate="G" pin="AN20" pad="44"/>
<connect gate="G" pin="AN21" pad="43"/>
<connect gate="G" pin="AN22" pad="42"/>
<connect gate="G" pin="AN23" pad="41"/>
<connect gate="G" pin="AN24" pad="40"/>
<connect gate="G" pin="AN25" pad="39"/>
<connect gate="G" pin="AN26" pad="38"/>
<connect gate="G" pin="AN27" pad="37"/>
<connect gate="G" pin="AN28" pad="35"/>
<connect gate="G" pin="AN29" pad="34"/>
<connect gate="G" pin="AN3" pad="64"/>
<connect gate="G" pin="AN30" pad="33"/>
<connect gate="G" pin="AN31" pad="32"/>
<connect gate="G" pin="AN32" pad="31"/>
<connect gate="G" pin="AN33" pad="30"/>
<connect gate="G" pin="AN34" pad="29"/>
<connect gate="G" pin="AN35" pad="28"/>
<connect gate="G" pin="AN4" pad="63"/>
<connect gate="G" pin="AN5" pad="62"/>
<connect gate="G" pin="AN6" pad="61"/>
<connect gate="G" pin="AN7" pad="36"/>
<connect gate="G" pin="AN8" pad="60"/>
<connect gate="G" pin="AN9" pad="59"/>
<connect gate="G" pin="BYPASS" pad="119"/>
<connect gate="G" pin="FCLN0" pad="156"/>
<connect gate="G" pin="FCLP0A" pad="157"/>
<connect gate="G" pin="NC@0" pad="21"/>
<connect gate="G" pin="NC@1" pad="89"/>
<connect gate="G" pin="P0.0" pad="145"/>
<connect gate="G" pin="P0.1" pad="146"/>
<connect gate="G" pin="P0.10" pad="151"/>
<connect gate="G" pin="P0.11" pad="152"/>
<connect gate="G" pin="P0.12" pad="168"/>
<connect gate="G" pin="P0.13" pad="169"/>
<connect gate="G" pin="P0.14" pad="175"/>
<connect gate="G" pin="P0.15" pad="176"/>
<connect gate="G" pin="P0.2" pad="147"/>
<connect gate="G" pin="P0.3" pad="148"/>
<connect gate="G" pin="P0.4" pad="166"/>
<connect gate="G" pin="P0.5" pad="167"/>
<connect gate="G" pin="P0.6" pad="173"/>
<connect gate="G" pin="P0.7" pad="174"/>
<connect gate="G" pin="P0.8" pad="149"/>
<connect gate="G" pin="P0.9" pad="150"/>
<connect gate="G" pin="P1.0" pad="91"/>
<connect gate="G" pin="P1.1" pad="92"/>
<connect gate="G" pin="P1.10" pad="96"/>
<connect gate="G" pin="P1.11" pad="97"/>
<connect gate="G" pin="P1.12" pad="73"/>
<connect gate="G" pin="P1.13" pad="72"/>
<connect gate="G" pin="P1.14" pad="71"/>
<connect gate="G" pin="P1.2" pad="93"/>
<connect gate="G" pin="P1.3" pad="98"/>
<connect gate="G" pin="P1.4" pad="107"/>
<connect gate="G" pin="P1.5" pad="108"/>
<connect gate="G" pin="P1.6" pad="109"/>
<connect gate="G" pin="P1.7" pad="110"/>
<connect gate="G" pin="P1.8" pad="94"/>
<connect gate="G" pin="P1.9" pad="95"/>
<connect gate="G" pin="P2.0" pad="74"/>
<connect gate="G" pin="P2.1" pad="75"/>
<connect gate="G" pin="P2.10" pad="161"/>
<connect gate="G" pin="P2.11" pad="162"/>
<connect gate="G" pin="P2.12" pad="163"/>
<connect gate="G" pin="P2.13" pad="165"/>
<connect gate="G" pin="P2.2" pad="76"/>
<connect gate="G" pin="P2.3" pad="77"/>
<connect gate="G" pin="P2.4" pad="78"/>
<connect gate="G" pin="P2.5" pad="79"/>
<connect gate="G" pin="P2.6" pad="80"/>
<connect gate="G" pin="P2.7" pad="81"/>
<connect gate="G" pin="P2.8" pad="164"/>
<connect gate="G" pin="P2.9" pad="160"/>
<connect gate="G" pin="P3.0" pad="136"/>
<connect gate="G" pin="P3.1" pad="135"/>
<connect gate="G" pin="P3.10" pad="137"/>
<connect gate="G" pin="P3.11" pad="144"/>
<connect gate="G" pin="P3.12" pad="143"/>
<connect gate="G" pin="P3.13" pad="142"/>
<connect gate="G" pin="P3.14" pad="134"/>
<connect gate="G" pin="P3.15" pad="133"/>
<connect gate="G" pin="P3.2" pad="129"/>
<connect gate="G" pin="P3.3" pad="130"/>
<connect gate="G" pin="P3.4" pad="132"/>
<connect gate="G" pin="P3.5" pad="126"/>
<connect gate="G" pin="P3.6" pad="127"/>
<connect gate="G" pin="P3.7" pad="131"/>
<connect gate="G" pin="P3.8" pad="128"/>
<connect gate="G" pin="P3.9" pad="138"/>
<connect gate="G" pin="P4.0" pad="86"/>
<connect gate="G" pin="P4.1" pad="87"/>
<connect gate="G" pin="P4.2" pad="88"/>
<connect gate="G" pin="P4.3" pad="90"/>
<connect gate="G" pin="P5.0" pad="1"/>
<connect gate="G" pin="P5.1" pad="2"/>
<connect gate="G" pin="P5.10" pad="15"/>
<connect gate="G" pin="P5.11" pad="16"/>
<connect gate="G" pin="P5.12" pad="17"/>
<connect gate="G" pin="P5.13" pad="18"/>
<connect gate="G" pin="P5.14" pad="19"/>
<connect gate="G" pin="P5.15" pad="20"/>
<connect gate="G" pin="P5.2" pad="3"/>
<connect gate="G" pin="P5.3" pad="4"/>
<connect gate="G" pin="P5.4" pad="5"/>
<connect gate="G" pin="P5.5" pad="6"/>
<connect gate="G" pin="P5.6" pad="7"/>
<connect gate="G" pin="P5.7" pad="8"/>
<connect gate="G" pin="P5.8" pad="13"/>
<connect gate="G" pin="P5.9" pad="14"/>
<connect gate="G" pin="SON0" pad="158"/>
<connect gate="G" pin="SOP0A" pad="159"/>
<connect gate="G" pin="TCK" pad="115"/>
<connect gate="G" pin="TDI" pad="111"/>
<connect gate="G" pin="TDO" pad="113"/>
<connect gate="G" pin="TMS" pad="112"/>
<connect gate="G" pin="TRCLK" pad="9"/>
<connect gate="G" pin="XTAL1" pad="102"/>
<connect gate="G" pin="XTAL2" pad="103"/>
<connect gate="PWR" pin="VAGND" pad="27"/>
<connect gate="PWR" pin="VAGND0" pad="51"/>
<connect gate="PWR" pin="VAREF" pad="26"/>
<connect gate="PWR" pin="VAREF0" pad="52"/>
<connect gate="PWR" pin="VDD@0" pad="10"/>
<connect gate="PWR" pin="VDD@1" pad="68"/>
<connect gate="PWR" pin="VDD@2" pad="84"/>
<connect gate="PWR" pin="VDD@3" pad="99"/>
<connect gate="PWR" pin="VDD@4" pad="123"/>
<connect gate="PWR" pin="VDD@5" pad="153"/>
<connect gate="PWR" pin="VDD@6" pad="170"/>
<connect gate="PWR" pin="VDDAF" pad="23"/>
<connect gate="PWR" pin="VDDFL3" pad="141"/>
<connect gate="PWR" pin="VDDM" pad="54"/>
<connect gate="PWR" pin="VDDMF" pad="24"/>
<connect gate="PWR" pin="VDDOSC" pad="105"/>
<connect gate="PWR" pin="VDDOSC3" pad="106"/>
<connect gate="PWR" pin="VDDP@0" pad="11"/>
<connect gate="PWR" pin="VDDP@1" pad="69"/>
<connect gate="PWR" pin="VDDP@2" pad="83"/>
<connect gate="PWR" pin="VDDP@3" pad="100"/>
<connect gate="PWR" pin="VDDP@4" pad="124"/>
<connect gate="PWR" pin="VDDP@5" pad="154"/>
<connect gate="PWR" pin="VDDP@6" pad="171"/>
<connect gate="PWR" pin="VDDP@7" pad="139"/>
<connect gate="PWR" pin="VSS@0" pad="12"/>
<connect gate="PWR" pin="VSS@1" pad="70"/>
<connect gate="PWR" pin="VSS@2" pad="85"/>
<connect gate="PWR" pin="VSS@3" pad="101"/>
<connect gate="PWR" pin="VSS@4" pad="125"/>
<connect gate="PWR" pin="VSS@5" pad="155"/>
<connect gate="PWR" pin="VSS@6" pad="172"/>
<connect gate="PWR" pin="VSS@7" pad="140"/>
<connect gate="PWR" pin="VSS@8" pad="82"/>
<connect gate="PWR" pin="VSSAF" pad="22"/>
<connect gate="PWR" pin="VSSM" pad="53"/>
<connect gate="PWR" pin="VSSMF" pad="25"/>
<connect gate="PWR" pin="VSSOSC" pad="104"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAK-TC1796" prefix="IC">
<description>&lt;b&gt; TC1796 32-Bit Single Chip Microcontroller &lt;/b&gt;</description>
<gates>
<gate name="JTAG" symbol="TC1796JTAG"/>
<gate name="P2" symbol="TC1796-P2"/>
<gate name="P3/GPTA" symbol="TC1796P3"/>
<gate name="P4/GPTA" symbol="TC1796P4"/>
<gate name="P5" symbol="TC1796P5"/>
<gate name="P6" symbol="TC1796P6"/>
<gate name="DIGITALPOWER" symbol="TC1796PWRD"/>
<gate name="PWR" symbol="TC1796PWRA"/>
<gate name="AN" symbol="TC1796AN"/>
<gate name="G" symbol="TC1796"/>
<gate name="NC" symbol="TC1796NC"/>
</gates>
<devices>
<device name="" package="P-BGA-416">
<connects>
<connect gate="AN" pin="AN0" pad="AE1"/>
<connect gate="AN" pin="AN1" pad="AD2"/>
<connect gate="AN" pin="AN10" pad="Y3"/>
<connect gate="AN" pin="AN11" pad="AA2"/>
<connect gate="AN" pin="AN12" pad="AB1"/>
<connect gate="AN" pin="AN13" pad="W3"/>
<connect gate="AN" pin="AN14" pad="Y2"/>
<connect gate="AN" pin="AN15" pad="AA1"/>
<connect gate="AN" pin="AN16" pad="V4"/>
<connect gate="AN" pin="AN17" pad="W2"/>
<connect gate="AN" pin="AN18" pad="Y1"/>
<connect gate="AN" pin="AN19" pad="V3"/>
<connect gate="AN" pin="AN2" pad="AA4"/>
<connect gate="AN" pin="AN20" pad="W1"/>
<connect gate="AN" pin="AN21" pad="V2"/>
<connect gate="AN" pin="AN22" pad="V1"/>
<connect gate="AN" pin="AN23" pad="U1"/>
<connect gate="AN" pin="AN24" pad="AC8"/>
<connect gate="AN" pin="AN25" pad="AD8"/>
<connect gate="AN" pin="AN26" pad="AC7"/>
<connect gate="AN" pin="AN27" pad="AD7"/>
<connect gate="AN" pin="AN28" pad="AE6"/>
<connect gate="AN" pin="AN29" pad="AF6"/>
<connect gate="AN" pin="AN3" pad="AB3"/>
<connect gate="AN" pin="AN30" pad="AE7"/>
<connect gate="AN" pin="AN31" pad="AF7"/>
<connect gate="AN" pin="AN32" pad="AC3"/>
<connect gate="AN" pin="AN33" pad="AE2"/>
<connect gate="AN" pin="AN34" pad="AD3"/>
<connect gate="AN" pin="AN35" pad="AD5"/>
<connect gate="AN" pin="AN36" pad="AE3"/>
<connect gate="AN" pin="AN37" pad="AF2"/>
<connect gate="AN" pin="AN38" pad="AC4"/>
<connect gate="AN" pin="AN39" pad="AF3"/>
<connect gate="AN" pin="AN4" pad="AC2"/>
<connect gate="AN" pin="AN40" pad="AD4"/>
<connect gate="AN" pin="AN41" pad="AE4"/>
<connect gate="AN" pin="AN42" pad="AC5"/>
<connect gate="AN" pin="AN43" pad="AF4"/>
<connect gate="AN" pin="AN5" pad="AA3"/>
<connect gate="AN" pin="AN6" pad="AD1"/>
<connect gate="AN" pin="AN7" pad="AB4"/>
<connect gate="AN" pin="AN8" pad="AC1"/>
<connect gate="AN" pin="AN9" pad="AB2"/>
<connect gate="DIGITALPOWER" pin="VDD@0" pad="B26"/>
<connect gate="DIGITALPOWER" pin="VDD@1" pad="C25"/>
<connect gate="DIGITALPOWER" pin="VDD@10" pad="AB23"/>
<connect gate="DIGITALPOWER" pin="VDD@11" pad="AC11"/>
<connect gate="DIGITALPOWER" pin="VDD@12" pad="AC20"/>
<connect gate="DIGITALPOWER" pin="VDD@2" pad="D9"/>
<connect gate="DIGITALPOWER" pin="VDD@3" pad="D16"/>
<connect gate="DIGITALPOWER" pin="VDD@4" pad="D24"/>
<connect gate="DIGITALPOWER" pin="VDD@5" pad="E23"/>
<connect gate="DIGITALPOWER" pin="VDD@6" pad="H4"/>
<connect gate="DIGITALPOWER" pin="VDD@7" pad="P23"/>
<connect gate="DIGITALPOWER" pin="VDD@8" pad="R4"/>
<connect gate="DIGITALPOWER" pin="VDD@9" pad="V23"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@0" pad="H23"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@1" pad="H24"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@2" pad="H25"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@3" pad="H26"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@4" pad="M23"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@5" pad="T23"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@6" pad="Y23"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@7" pad="AC18"/>
<connect gate="DIGITALPOWER" pin="VDDEBU@8" pad="AC22"/>
<connect gate="DIGITALPOWER" pin="VDDFL3@0" pad="A18"/>
<connect gate="DIGITALPOWER" pin="VDDFL3@1" pad="B18"/>
<connect gate="DIGITALPOWER" pin="VDDP@0" pad="A25"/>
<connect gate="DIGITALPOWER" pin="VDDP@1" pad="B24"/>
<connect gate="DIGITALPOWER" pin="VDDP@10" pad="AF16"/>
<connect gate="DIGITALPOWER" pin="VDDP@2" pad="C23"/>
<connect gate="DIGITALPOWER" pin="VDDP@3" pad="D7"/>
<connect gate="DIGITALPOWER" pin="VDDP@4" pad="D14"/>
<connect gate="DIGITALPOWER" pin="VDDP@5" pad="D22"/>
<connect gate="DIGITALPOWER" pin="VDDP@6" pad="K4"/>
<connect gate="DIGITALPOWER" pin="VDDP@7" pad="AC16"/>
<connect gate="DIGITALPOWER" pin="VDDP@8" pad="AD16"/>
<connect gate="DIGITALPOWER" pin="VDDP@9" pad="AE16"/>
<connect gate="DIGITALPOWER" pin="VDDSBRAM" pad="R1"/>
<connect gate="DIGITALPOWER" pin="VSS@0" pad="D8"/>
<connect gate="DIGITALPOWER" pin="VSS@1" pad="D15"/>
<connect gate="DIGITALPOWER" pin="VSS@10" pad="AC23"/>
<connect gate="DIGITALPOWER" pin="VSS@11" pad="AC19"/>
<connect gate="DIGITALPOWER" pin="VSS@12" pad="AC17"/>
<connect gate="DIGITALPOWER" pin="VSS@13" pad="AC10"/>
<connect gate="DIGITALPOWER" pin="VSS@14" pad="T4"/>
<connect gate="DIGITALPOWER" pin="VSS@15" pad="K17"/>
<connect gate="DIGITALPOWER" pin="VSS@16" pad="K16"/>
<connect gate="DIGITALPOWER" pin="VSS@17" pad="K15"/>
<connect gate="DIGITALPOWER" pin="VSS@18" pad="K14"/>
<connect gate="DIGITALPOWER" pin="VSS@19" pad="K13"/>
<connect gate="DIGITALPOWER" pin="VSS@2" pad="D23"/>
<connect gate="DIGITALPOWER" pin="VSS@20" pad="L17"/>
<connect gate="DIGITALPOWER" pin="VSS@21" pad="L16"/>
<connect gate="DIGITALPOWER" pin="VSS@22" pad="L15"/>
<connect gate="DIGITALPOWER" pin="VSS@23" pad="L14"/>
<connect gate="DIGITALPOWER" pin="VSS@24" pad="L13"/>
<connect gate="DIGITALPOWER" pin="VSS@25" pad="M17"/>
<connect gate="DIGITALPOWER" pin="VSS@26" pad="M16"/>
<connect gate="DIGITALPOWER" pin="VSS@27" pad="M15"/>
<connect gate="DIGITALPOWER" pin="VSS@28" pad="M14"/>
<connect gate="DIGITALPOWER" pin="VSS@29" pad="M13"/>
<connect gate="DIGITALPOWER" pin="VSS@3" pad="C24"/>
<connect gate="DIGITALPOWER" pin="VSS@30" pad="M12"/>
<connect gate="DIGITALPOWER" pin="VSS@31" pad="N17"/>
<connect gate="DIGITALPOWER" pin="VSS@32" pad="N16"/>
<connect gate="DIGITALPOWER" pin="VSS@33" pad="N15"/>
<connect gate="DIGITALPOWER" pin="VSS@34" pad="N14"/>
<connect gate="DIGITALPOWER" pin="VSS@35" pad="N13"/>
<connect gate="DIGITALPOWER" pin="VSS@36" pad="N12"/>
<connect gate="DIGITALPOWER" pin="VSS@37" pad="N11"/>
<connect gate="DIGITALPOWER" pin="VSS@38" pad="N10"/>
<connect gate="DIGITALPOWER" pin="VSS@39" pad="P17"/>
<connect gate="DIGITALPOWER" pin="VSS@4" pad="B25"/>
<connect gate="DIGITALPOWER" pin="VSS@40" pad="P16"/>
<connect gate="DIGITALPOWER" pin="VSS@41" pad="P15"/>
<connect gate="DIGITALPOWER" pin="VSS@42" pad="P14"/>
<connect gate="DIGITALPOWER" pin="VSS@43" pad="P13"/>
<connect gate="DIGITALPOWER" pin="VSS@44" pad="P12"/>
<connect gate="DIGITALPOWER" pin="VSS@45" pad="P11"/>
<connect gate="DIGITALPOWER" pin="VSS@46" pad="P10"/>
<connect gate="DIGITALPOWER" pin="VSS@47" pad="R17"/>
<connect gate="DIGITALPOWER" pin="VSS@48" pad="R16"/>
<connect gate="DIGITALPOWER" pin="VSS@49" pad="R15"/>
<connect gate="DIGITALPOWER" pin="VSS@5" pad="A26"/>
<connect gate="DIGITALPOWER" pin="VSS@50" pad="R14"/>
<connect gate="DIGITALPOWER" pin="VSS@51" pad="R13"/>
<connect gate="DIGITALPOWER" pin="VSS@52" pad="T17"/>
<connect gate="DIGITALPOWER" pin="VSS@53" pad="T16"/>
<connect gate="DIGITALPOWER" pin="VSS@54" pad="T15"/>
<connect gate="DIGITALPOWER" pin="VSS@55" pad="T14"/>
<connect gate="DIGITALPOWER" pin="VSS@56" pad="T13"/>
<connect gate="DIGITALPOWER" pin="VSS@57" pad="U17"/>
<connect gate="DIGITALPOWER" pin="VSS@58" pad="U16"/>
<connect gate="DIGITALPOWER" pin="VSS@59" pad="U15"/>
<connect gate="DIGITALPOWER" pin="VSS@6" pad="J4"/>
<connect gate="DIGITALPOWER" pin="VSS@60" pad="U14"/>
<connect gate="DIGITALPOWER" pin="VSS@61" pad="U13"/>
<connect gate="DIGITALPOWER" pin="VSS@7" pad="L23"/>
<connect gate="DIGITALPOWER" pin="VSS@8" pad="R23"/>
<connect gate="DIGITALPOWER" pin="VSS@9" pad="W23"/>
<connect gate="G" pin="!ADV" pad="AF22"/>
<connect gate="G" pin="!BAA" pad="AF23"/>
<connect gate="G" pin="!BC0" pad="AE17"/>
<connect gate="G" pin="!BC1" pad="AD17"/>
<connect gate="G" pin="!BC2" pad="AF18"/>
<connect gate="G" pin="!BC3" pad="AE18"/>
<connect gate="G" pin="!BREQ" pad="AD22"/>
<connect gate="G" pin="!CSEL0" pad="AE21"/>
<connect gate="G" pin="!CSEL1" pad="AD21"/>
<connect gate="G" pin="!CSEL2" pad="AD20"/>
<connect gate="G" pin="!CSEL3" pad="AD19"/>
<connect gate="G" pin="!CSEL4" pad="AE19"/>
<connect gate="G" pin="!HDRST" pad="A23"/>
<connect gate="G" pin="!HLDA" pad="AD18"/>
<connect gate="G" pin="!HOLD" pad="AF17"/>
<connect gate="G" pin="!MR/!W" pad="AF19"/>
<connect gate="G" pin="!NMI" pad="A22"/>
<connect gate="G" pin="!PORST" pad="B22"/>
<connect gate="G" pin="!RD" pad="AF20"/>
<connect gate="G" pin="!RD/!WR" pad="AF21"/>
<connect gate="G" pin="!WAIT" pad="AE20"/>
<connect gate="G" pin="A0" pad="J24"/>
<connect gate="G" pin="A1" pad="J25"/>
<connect gate="G" pin="A10" pad="M26"/>
<connect gate="G" pin="A11" pad="M25"/>
<connect gate="G" pin="A12" pad="M24"/>
<connect gate="G" pin="A13" pad="L24"/>
<connect gate="G" pin="A14" pad="N26"/>
<connect gate="G" pin="A15" pad="N23"/>
<connect gate="G" pin="A16" pad="N24"/>
<connect gate="G" pin="A17" pad="N25"/>
<connect gate="G" pin="A18" pad="P26"/>
<connect gate="G" pin="A19" pad="P24"/>
<connect gate="G" pin="A2" pad="J26"/>
<connect gate="G" pin="A20" pad="P25"/>
<connect gate="G" pin="A21" pad="R24"/>
<connect gate="G" pin="A22" pad="R26"/>
<connect gate="G" pin="A23" pad="R25"/>
<connect gate="G" pin="A3" pad="K25"/>
<connect gate="G" pin="A4" pad="K26"/>
<connect gate="G" pin="A5" pad="J23"/>
<connect gate="G" pin="A6" pad="K24"/>
<connect gate="G" pin="A7" pad="L25"/>
<connect gate="G" pin="A8" pad="L26"/>
<connect gate="G" pin="A9" pad="K23"/>
<connect gate="G" pin="BFCLKI" pad="AF24"/>
<connect gate="G" pin="BFLCKO" pad="AF25"/>
<connect gate="G" pin="BYPASS" pad="A24"/>
<connect gate="G" pin="D0" pad="T26"/>
<connect gate="G" pin="D1" pad="T24"/>
<connect gate="G" pin="D10" pad="Y26"/>
<connect gate="G" pin="D11" pad="AA26"/>
<connect gate="G" pin="D12" pad="W25"/>
<connect gate="G" pin="D13" pad="V24"/>
<connect gate="G" pin="D14" pad="Y25"/>
<connect gate="G" pin="D15" pad="AB26"/>
<connect gate="G" pin="D16" pad="W24"/>
<connect gate="G" pin="D17" pad="AA25"/>
<connect gate="G" pin="D18" pad="Y24"/>
<connect gate="G" pin="D19" pad="AA23"/>
<connect gate="G" pin="D2" pad="U26"/>
<connect gate="G" pin="D20" pad="AB25"/>
<connect gate="G" pin="D21" pad="AB24"/>
<connect gate="G" pin="D22" pad="AA24"/>
<connect gate="G" pin="D23" pad="AC26"/>
<connect gate="G" pin="D24" pad="AD26"/>
<connect gate="G" pin="D25" pad="AC25"/>
<connect gate="G" pin="D26" pad="AE26"/>
<connect gate="G" pin="D27" pad="AD25"/>
<connect gate="G" pin="D28" pad="AC24"/>
<connect gate="G" pin="D29" pad="AE25"/>
<connect gate="G" pin="D3" pad="T25"/>
<connect gate="G" pin="D30" pad="AE24"/>
<connect gate="G" pin="D31" pad="AD24"/>
<connect gate="G" pin="D4" pad="V26"/>
<connect gate="G" pin="D5" pad="U25"/>
<connect gate="G" pin="D6" pad="U23"/>
<connect gate="G" pin="D7" pad="W26"/>
<connect gate="G" pin="D8" pad="V25"/>
<connect gate="G" pin="D9" pad="U24"/>
<connect gate="G" pin="FCLN0" pad="C17"/>
<connect gate="G" pin="FCLN1" pad="B17"/>
<connect gate="G" pin="FCLP0A" pad="C18"/>
<connect gate="G" pin="FCLP1A" pad="A17"/>
<connect gate="G" pin="MRST0" pad="AE15"/>
<connect gate="G" pin="MTSR0" pad="AF15"/>
<connect gate="G" pin="P0.0" pad="A9"/>
<connect gate="G" pin="P0.1" pad="A8"/>
<connect gate="G" pin="P0.10" pad="C6"/>
<connect gate="G" pin="P0.11" pad="D6"/>
<connect gate="G" pin="P0.12" pad="C5"/>
<connect gate="G" pin="P0.13" pad="D5"/>
<connect gate="G" pin="P0.14" pad="A5"/>
<connect gate="G" pin="P0.15" pad="D4"/>
<connect gate="G" pin="P0.2" pad="A7"/>
<connect gate="G" pin="P0.3" pad="B8"/>
<connect gate="G" pin="P0.4" pad="B7"/>
<connect gate="G" pin="P0.5" pad="A6"/>
<connect gate="G" pin="P0.6" pad="B6"/>
<connect gate="G" pin="P0.7" pad="C8"/>
<connect gate="G" pin="P0.8" pad="C7"/>
<connect gate="G" pin="P0.9" pad="B5"/>
<connect gate="G" pin="P1.0" pad="P3"/>
<connect gate="G" pin="P1.1" pad="P2"/>
<connect gate="G" pin="P1.10" pad="M1"/>
<connect gate="G" pin="P1.11" pad="L4"/>
<connect gate="G" pin="P1.12" pad="P4"/>
<connect gate="G" pin="P1.13" pad="L3"/>
<connect gate="G" pin="P1.14" pad="L2"/>
<connect gate="G" pin="P1.15" pad="L1"/>
<connect gate="G" pin="P1.2" pad="P1"/>
<connect gate="G" pin="P1.3" pad="N1"/>
<connect gate="G" pin="P1.4" pad="N4"/>
<connect gate="G" pin="P1.5" pad="M4"/>
<connect gate="G" pin="P1.6" pad="N3"/>
<connect gate="G" pin="P1.7" pad="N2"/>
<connect gate="G" pin="P1.8" pad="M3"/>
<connect gate="G" pin="P1.9" pad="M2"/>
<connect gate="G" pin="P10.0/HWCFG.0" pad="A21"/>
<connect gate="G" pin="P10.1/HWCFG.1" pad="B21"/>
<connect gate="G" pin="P10.2/HWCFG.2" pad="C21"/>
<connect gate="G" pin="P10.3/HWCFG.3" pad="D21"/>
<connect gate="G" pin="P7.0" pad="R3"/>
<connect gate="G" pin="P7.1" pad="R2"/>
<connect gate="G" pin="P7.2" pad="U4"/>
<connect gate="G" pin="P7.3" pad="U3"/>
<connect gate="G" pin="P7.4" pad="T3"/>
<connect gate="G" pin="P7.5" pad="T2"/>
<connect gate="G" pin="P7.6" pad="T1"/>
<connect gate="G" pin="P7.7" pad="U2"/>
<connect gate="G" pin="P8.0" pad="H2"/>
<connect gate="G" pin="P8.1" pad="H1"/>
<connect gate="G" pin="P8.2" pad="J3"/>
<connect gate="G" pin="P8.3" pad="J2"/>
<connect gate="G" pin="P8.4" pad="J1"/>
<connect gate="G" pin="P8.5" pad="K2"/>
<connect gate="G" pin="P8.6" pad="K3"/>
<connect gate="G" pin="P8.7" pad="K1"/>
<connect gate="G" pin="P9.0" pad="A19"/>
<connect gate="G" pin="P9.1" pad="B19"/>
<connect gate="G" pin="P9.2" pad="B20"/>
<connect gate="G" pin="P9.3" pad="A20"/>
<connect gate="G" pin="P9.4" pad="D18"/>
<connect gate="G" pin="P9.5" pad="D19"/>
<connect gate="G" pin="P9.6" pad="C19"/>
<connect gate="G" pin="P9.7" pad="D20"/>
<connect gate="G" pin="P9.8" pad="C20"/>
<connect gate="G" pin="SCLK0" pad="AF14"/>
<connect gate="G" pin="SLSIO" pad="AD15"/>
<connect gate="G" pin="SLSO0" pad="AE14"/>
<connect gate="G" pin="SLSO1" pad="AC15"/>
<connect gate="G" pin="SON0" pad="D17"/>
<connect gate="G" pin="SON1" pad="A16"/>
<connect gate="G" pin="SOP0A" pad="C16"/>
<connect gate="G" pin="SOP1A" pad="B16"/>
<connect gate="G" pin="TESTMODE" pad="B23"/>
<connect gate="G" pin="TSTRES" pad="G24"/>
<connect gate="G" pin="VDDOSC-1.5V" pad="F26"/>
<connect gate="G" pin="VDDOSC-3V" pad="E26"/>
<connect gate="G" pin="VSSOSC" pad="F25"/>
<connect gate="G" pin="XTAL1" pad="G26"/>
<connect gate="G" pin="XTAL2" pad="G25"/>
<connect gate="JTAG" pin="!BRKIN" pad="C26"/>
<connect gate="JTAG" pin="!BRKOUT" pad="D26"/>
<connect gate="JTAG" pin="!TRST" pad="F23"/>
<connect gate="JTAG" pin="TCK" pad="E24"/>
<connect gate="JTAG" pin="TDI" pad="E25"/>
<connect gate="JTAG" pin="TDO" pad="D25"/>
<connect gate="JTAG" pin="TMS" pad="F24"/>
<connect gate="JTAG" pin="TR.0" pad="U12"/>
<connect gate="JTAG" pin="TR.1" pad="T12"/>
<connect gate="JTAG" pin="TR.10" pad="L11"/>
<connect gate="JTAG" pin="TR.11" pad="L10"/>
<connect gate="JTAG" pin="TR.12" pad="K10"/>
<connect gate="JTAG" pin="TR.13" pad="K11"/>
<connect gate="JTAG" pin="TR.14" pad="L12"/>
<connect gate="JTAG" pin="TR.15" pad="K12"/>
<connect gate="JTAG" pin="TR.2" pad="U11"/>
<connect gate="JTAG" pin="TR.3" pad="T11"/>
<connect gate="JTAG" pin="TR.4" pad="U10"/>
<connect gate="JTAG" pin="TR.5" pad="R12"/>
<connect gate="JTAG" pin="TR.6" pad="R10"/>
<connect gate="JTAG" pin="TR.7" pad="R11"/>
<connect gate="JTAG" pin="TR.8" pad="M11"/>
<connect gate="JTAG" pin="TR.9" pad="M10"/>
<connect gate="JTAG" pin="TRCLK" pad="T10"/>
<connect gate="NC" pin="NC@0" pad="A1"/>
<connect gate="NC" pin="NC@1" pad="C22"/>
<connect gate="NC" pin="NC@2" pad="G23"/>
<connect gate="NC" pin="NC@3" pad="H3"/>
<connect gate="NC" pin="NC@4" pad="AF1"/>
<connect gate="NC" pin="NC@5" pad="AF26"/>
<connect gate="NC" pin="NC@6" pad="AC21"/>
<connect gate="NC" pin="NC@7" pad="AD23"/>
<connect gate="NC" pin="NC@8" pad="AE22"/>
<connect gate="NC" pin="NC@9" pad="AE23"/>
<connect gate="P2" pin="P2.10" pad="B3"/>
<connect gate="P2" pin="P2.11" pad="C3"/>
<connect gate="P2" pin="P2.12" pad="C4"/>
<connect gate="P2" pin="P2.13" pad="A3"/>
<connect gate="P2" pin="P2.14" pad="B4"/>
<connect gate="P2" pin="P2.15" pad="A4"/>
<connect gate="P2" pin="P2.2" pad="D3"/>
<connect gate="P2" pin="P2.3" pad="D2"/>
<connect gate="P2" pin="P2.4" pad="D1"/>
<connect gate="P2" pin="P2.5" pad="C1"/>
<connect gate="P2" pin="P2.6" pad="B1"/>
<connect gate="P2" pin="P2.7" pad="B2"/>
<connect gate="P2" pin="P2.8" pad="C2"/>
<connect gate="P2" pin="P2.9" pad="A2"/>
<connect gate="P3/GPTA" pin="P3.0" pad="B12"/>
<connect gate="P3/GPTA" pin="P3.1" pad="A12"/>
<connect gate="P3/GPTA" pin="P3.10" pad="C10"/>
<connect gate="P3/GPTA" pin="P3.11" pad="D13"/>
<connect gate="P3/GPTA" pin="P3.12" pad="D11"/>
<connect gate="P3/GPTA" pin="P3.13" pad="D12"/>
<connect gate="P3/GPTA" pin="P3.14" pad="A10"/>
<connect gate="P3/GPTA" pin="P3.15" pad="B9"/>
<connect gate="P3/GPTA" pin="P3.2" pad="C13"/>
<connect gate="P3/GPTA" pin="P3.3" pad="B11"/>
<connect gate="P3/GPTA" pin="P3.4" pad="C12"/>
<connect gate="P3/GPTA" pin="P3.5" pad="A11"/>
<connect gate="P3/GPTA" pin="P3.6" pad="B10"/>
<connect gate="P3/GPTA" pin="P3.7" pad="C9"/>
<connect gate="P3/GPTA" pin="P3.8" pad="D10"/>
<connect gate="P3/GPTA" pin="P3.9" pad="C11"/>
<connect gate="P4/GPTA" pin="P4.0" pad="AD10"/>
<connect gate="P4/GPTA" pin="P4.1" pad="AE10"/>
<connect gate="P4/GPTA" pin="P4.10" pad="AF12"/>
<connect gate="P4/GPTA" pin="P4.11" pad="AD13"/>
<connect gate="P4/GPTA" pin="P4.12" pad="AC14"/>
<connect gate="P4/GPTA" pin="P4.13" pad="AE13"/>
<connect gate="P4/GPTA" pin="P4.14" pad="AF13"/>
<connect gate="P4/GPTA" pin="P4.15" pad="AD14"/>
<connect gate="P4/GPTA" pin="P4.2" pad="AD11"/>
<connect gate="P4/GPTA" pin="P4.3" pad="AE11"/>
<connect gate="P4/GPTA" pin="P4.4" pad="AC12"/>
<connect gate="P4/GPTA" pin="P4.5" pad="AD12"/>
<connect gate="P4/GPTA" pin="P4.6" pad="AF10"/>
<connect gate="P4/GPTA" pin="P4.7" pad="AE12"/>
<connect gate="P4/GPTA" pin="P4.8" pad="AC13"/>
<connect gate="P4/GPTA" pin="P4.9" pad="AF11"/>
<connect gate="P5" pin="P5.0" pad="B13"/>
<connect gate="P5" pin="P5.1" pad="A13"/>
<connect gate="P5" pin="P5.2" pad="A14"/>
<connect gate="P5" pin="P5.3" pad="B14"/>
<connect gate="P5" pin="P5.4" pad="C15"/>
<connect gate="P5" pin="P5.5" pad="C14"/>
<connect gate="P5" pin="P5.6" pad="B15"/>
<connect gate="P5" pin="P5.7" pad="A15"/>
<connect gate="P6" pin="P6.10" pad="F2"/>
<connect gate="P6" pin="P6.11" pad="E2"/>
<connect gate="P6" pin="P6.12" pad="E1"/>
<connect gate="P6" pin="P6.13" pad="G2"/>
<connect gate="P6" pin="P6.14" pad="F1"/>
<connect gate="P6" pin="P6.15" pad="G1"/>
<connect gate="P6" pin="P6.4" pad="F3"/>
<connect gate="P6" pin="P6.5" pad="G4"/>
<connect gate="P6" pin="P6.6" pad="E3"/>
<connect gate="P6" pin="P6.7" pad="G3"/>
<connect gate="P6" pin="P6.8" pad="F4"/>
<connect gate="P6" pin="P6.9" pad="E4"/>
<connect gate="PWR" pin="VAGND@0" pad="AC6"/>
<connect gate="PWR" pin="VAGND@1" pad="AF5"/>
<connect gate="PWR" pin="VAREF@0" pad="AE5"/>
<connect gate="PWR" pin="VAREF@1" pad="AD6"/>
<connect gate="PWR" pin="VDDAF@0" pad="AC9"/>
<connect gate="PWR" pin="VDDM@0" pad="W4"/>
<connect gate="PWR" pin="VDDMF@0" pad="AE9"/>
<connect gate="PWR" pin="VFAGND@0" pad="AE8"/>
<connect gate="PWR" pin="VFAREF@0" pad="AF8"/>
<connect gate="PWR" pin="VSSAF@0" pad="AD9"/>
<connect gate="PWR" pin="VSSM@0" pad="Y4"/>
<connect gate="PWR" pin="VSSMF@0" pad="AF9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAK-TC1910*" prefix="IC">
<description>&lt;b&gt;32 bit TriCore based microcontroller/DSP&lt;/b&gt;&lt;p&gt;
 which is mainly designed for automotive telematics applications.&lt;br&gt;
Source: http://www.infineon.com .. TC1910_DS_V1.0.pdf / TC1912_DS_V1.0.pdf</description>
<gates>
<gate name="-C" symbol="TC1910"/>
<gate name="-JTAG" symbol="JTAG-OCSD"/>
<gate name="-P0" symbol="PORT0-10_12"/>
<gate name="-P1" symbol="PORT1-10_12"/>
<gate name="-P2" symbol="PORT2-10_12"/>
<gate name="-P3" symbol="PORT3-10_12"/>
<gate name="HS1" symbol="HEATSINK"/>
<gate name="HS2" symbol="HEATSINK"/>
<gate name="HS3" symbol="HEATSINK"/>
<gate name="HS4" symbol="HEATSINK"/>
<gate name="HS5" symbol="HEATSINK"/>
<gate name="HS6" symbol="HEATSINK"/>
<gate name="HS7" symbol="HEATSINK"/>
<gate name="HS8" symbol="HEATSINK"/>
<gate name="HS9" symbol="HEATSINK"/>
<gate name="HS10" symbol="HEATSINK"/>
<gate name="HS11" symbol="HEATSINK"/>
<gate name="HS12" symbol="HEATSINK"/>
<gate name="HS13" symbol="HEATSINK"/>
<gate name="HS14" symbol="HEATSINK"/>
<gate name="HS15" symbol="HEATSINK"/>
<gate name="HS0" symbol="HEATSINK"/>
<gate name="-A" symbol="A23"/>
<gate name="-AD" symbol="AD31"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="-A" pin="A0" pad="R3"/>
<connect gate="-A" pin="A1" pad="P4"/>
<connect gate="-A" pin="A10" pad="N1"/>
<connect gate="-A" pin="A11" pad="M4"/>
<connect gate="-A" pin="A12" pad="M3"/>
<connect gate="-A" pin="A13" pad="L4"/>
<connect gate="-A" pin="A14" pad="M2"/>
<connect gate="-A" pin="A15" pad="M1"/>
<connect gate="-A" pin="A16" pad="L3"/>
<connect gate="-A" pin="A17" pad="L1"/>
<connect gate="-A" pin="A18" pad="L2"/>
<connect gate="-A" pin="A19" pad="K4"/>
<connect gate="-A" pin="A2" pad="T1"/>
<connect gate="-A" pin="A20" pad="K3"/>
<connect gate="-A" pin="A21" pad="J4"/>
<connect gate="-A" pin="A22" pad="K2"/>
<connect gate="-A" pin="A23" pad="J3"/>
<connect gate="-A" pin="A3" pad="R2"/>
<connect gate="-A" pin="A4" pad="R1"/>
<connect gate="-A" pin="A5" pad="P3"/>
<connect gate="-A" pin="A6" pad="P2"/>
<connect gate="-A" pin="A7" pad="P1"/>
<connect gate="-A" pin="A8" pad="N3"/>
<connect gate="-A" pin="A9" pad="N2"/>
<connect gate="-AD" pin="AD0" pad="H4"/>
<connect gate="-AD" pin="AD1" pad="J2"/>
<connect gate="-AD" pin="AD10" pad="G3"/>
<connect gate="-AD" pin="AD11" pad="G2"/>
<connect gate="-AD" pin="AD12" pad="F4"/>
<connect gate="-AD" pin="AD13" pad="C1"/>
<connect gate="-AD" pin="AD14" pad="F3"/>
<connect gate="-AD" pin="AD15" pad="F2"/>
<connect gate="-AD" pin="AD16" pad="E3"/>
<connect gate="-AD" pin="AD17" pad="B1"/>
<connect gate="-AD" pin="AD18" pad="E2"/>
<connect gate="-AD" pin="AD19" pad="E4"/>
<connect gate="-AD" pin="AD2" pad="H1"/>
<connect gate="-AD" pin="AD20" pad="A1"/>
<connect gate="-AD" pin="AD21" pad="D2"/>
<connect gate="-AD" pin="AD22" pad="D3"/>
<connect gate="-AD" pin="AD23" pad="C2"/>
<connect gate="-AD" pin="AD24" pad="C3"/>
<connect gate="-AD" pin="AD25" pad="B2"/>
<connect gate="-AD" pin="AD26" pad="A2"/>
<connect gate="-AD" pin="AD27" pad="B3"/>
<connect gate="-AD" pin="AD28" pad="A3"/>
<connect gate="-AD" pin="AD29" pad="A4"/>
<connect gate="-AD" pin="AD3" pad="H3"/>
<connect gate="-AD" pin="AD30" pad="B4"/>
<connect gate="-AD" pin="AD31" pad="C4"/>
<connect gate="-AD" pin="AD4" pad="H2"/>
<connect gate="-AD" pin="AD5" pad="G1"/>
<connect gate="-AD" pin="AD6" pad="G4"/>
<connect gate="-AD" pin="AD7" pad="F1"/>
<connect gate="-AD" pin="AD8" pad="E1"/>
<connect gate="-AD" pin="AD9" pad="D1"/>
<connect gate="-C" pin="!ADV" pad="N9"/>
<connect gate="-C" pin="!BAA" pad="P8"/>
<connect gate="-C" pin="!BC0" pad="N6"/>
<connect gate="-C" pin="!BC1" pad="R5"/>
<connect gate="-C" pin="!BC2" pad="T4"/>
<connect gate="-C" pin="!BC3" pad="T3"/>
<connect gate="-C" pin="!CAS" pad="T2"/>
<connect gate="-C" pin="!CMDELAY" pad="T9"/>
<connect gate="-C" pin="!CS0" pad="R7"/>
<connect gate="-C" pin="!CS1" pad="N7"/>
<connect gate="-C" pin="!CS2" pad="P7"/>
<connect gate="-C" pin="!CS3" pad="T6"/>
<connect gate="-C" pin="!CS4" pad="R6"/>
<connect gate="-C" pin="!CS5" pad="T5"/>
<connect gate="-C" pin="!CS6" pad="P6"/>
<connect gate="-C" pin="!CSEMU" pad="R8"/>
<connect gate="-C" pin="!CSGLB" pad="N8"/>
<connect gate="-C" pin="!CSOVL" pad="T8"/>
<connect gate="-C" pin="!HRST" pad="B13"/>
<connect gate="-C" pin="!MR_W" pad="R9"/>
<connect gate="-C" pin="!NMI" pad="A13"/>
<connect gate="-C" pin="!PORST" pad="C13"/>
<connect gate="-C" pin="!RAS" pad="N5"/>
<connect gate="-C" pin="!RD" pad="R4"/>
<connect gate="-C" pin="!RD_WR" pad="P5"/>
<connect gate="-C" pin="!SCANMODE" pad="J14"/>
<connect gate="-C" pin="!WAIT" pad="T7"/>
<connect gate="-C" pin="AI0+" pad="D9"/>
<connect gate="-C" pin="AI0-" pad="B9"/>
<connect gate="-C" pin="AI1+" pad="C10"/>
<connect gate="-C" pin="AI1-" pad="B10"/>
<connect gate="-C" pin="ALE" pad="R10"/>
<connect gate="-C" pin="AO0+" pad="C11"/>
<connect gate="-C" pin="AO0-" pad="B12"/>
<connect gate="-C" pin="AO1+" pad="B11"/>
<connect gate="-C" pin="AO1-" pad="D11"/>
<connect gate="-C" pin="BFCLK0" pad="K1"/>
<connect gate="-C" pin="BYPASS" pad="A12"/>
<connect gate="-C" pin="CEXT" pad="D12"/>
<connect gate="-C" pin="CKE" pad="P9"/>
<connect gate="-C" pin="CLKOUT" pad="A14"/>
<connect gate="-C" pin="CODEC_DIS" pad="C12"/>
<connect gate="-C" pin="EBUCLK" pad="J1"/>
<connect gate="-C" pin="PLLCTRL_AO" pad="D8"/>
<connect gate="-C" pin="TM_CTRL0" pad="C7"/>
<connect gate="-C" pin="TM_CTRL1" pad="C5"/>
<connect gate="-C" pin="VAGND_GOD" pad="C9"/>
<connect gate="-C" pin="VAREF_GOD" pad="D10"/>
<connect gate="-C" pin="VDDPLL" pad="B6"/>
<connect gate="-C" pin="VDDR" pad="D6"/>
<connect gate="-C" pin="VDDSB" pad="L13"/>
<connect gate="-C" pin="VDD_COD0/1" pad="A10"/>
<connect gate="-C" pin="VDD_GUARD" pad="B8"/>
<connect gate="-C" pin="VDD_OSCI" pad="D7"/>
<connect gate="-C" pin="VDD_PLL" pad="A9"/>
<connect gate="-C" pin="VDD_PWR2@1" pad="G7"/>
<connect gate="-C" pin="VDD_PWR2@2" pad="G10"/>
<connect gate="-C" pin="VDD_PWR2@3" pad="K7"/>
<connect gate="-C" pin="VDD_PWR2@4" pad="K10"/>
<connect gate="-C" pin="VDD_PWR@1" pad="D4"/>
<connect gate="-C" pin="VDD_PWR@2" pad="D13"/>
<connect gate="-C" pin="VDD_PWR@3" pad="H7"/>
<connect gate="-C" pin="VDD_PWR@4" pad="N4"/>
<connect gate="-C" pin="VDD_PWR@5" pad="N13"/>
<connect gate="-C" pin="VDD_RTC" pad="A5"/>
<connect gate="-C" pin="VSSA_COD0/1" pad="A11"/>
<connect gate="-C" pin="VSSPLL" pad="A8"/>
<connect gate="-C" pin="VSS_32K" pad="B5"/>
<connect gate="-C" pin="VSS_GND@1" pad="G8"/>
<connect gate="-C" pin="VSS_GND@2" pad="G9"/>
<connect gate="-C" pin="VSS_GND@3" pad="H8"/>
<connect gate="-C" pin="VSS_GND@4" pad="H9"/>
<connect gate="-C" pin="VSS_GND@5" pad="J8"/>
<connect gate="-C" pin="VSS_GND@6" pad="J9"/>
<connect gate="-C" pin="VSS_GUARD" pad="C8"/>
<connect gate="-C" pin="VSS_PLL" pad="B7"/>
<connect gate="-C" pin="XTAL1" pad="A6"/>
<connect gate="-C" pin="XTAL2" pad="A7"/>
<connect gate="-C" pin="XTAL3" pad="D5"/>
<connect gate="-C" pin="XTAL4" pad="C6"/>
<connect gate="-JTAG" pin="!BRKIN" pad="R13"/>
<connect gate="-JTAG" pin="!BRKOUT" pad="P12"/>
<connect gate="-JTAG" pin="!OCDSE" pad="T14"/>
<connect gate="-JTAG" pin="!TRST" pad="T16"/>
<connect gate="-JTAG" pin="TCK" pad="R15"/>
<connect gate="-JTAG" pin="TDI" pad="T15"/>
<connect gate="-JTAG" pin="TDO" pad="R14"/>
<connect gate="-JTAG" pin="TMS" pad="P13"/>
<connect gate="-P0" pin="0/EXI0IN" pad="M14"/>
<connect gate="-P0" pin="1/EXI1IN/DATA_IN" pad="M15"/>
<connect gate="-P0" pin="2/EXI2IN/DATA_OUT" pad="M16"/>
<connect gate="-P0" pin="3/EXI3IN/MCLK" pad="L14"/>
<connect gate="-P0" pin="4/GPIO/SCLK" pad="L15"/>
<connect gate="-P0" pin="5/GPIO/LRCK" pad="K13"/>
<connect gate="-P0" pin="6/GPIO/MUTE0" pad="L16"/>
<connect gate="-P0" pin="7/GPIO/MUTE1" pad="K14"/>
<connect gate="-P1" pin="0/GPIO" pad="P14"/>
<connect gate="-P1" pin="1/GPIO" pad="R16"/>
<connect gate="-P1" pin="2/GPIO" pad="P15"/>
<connect gate="-P1" pin="3/GPIO" pad="P16"/>
<connect gate="-P1" pin="4/GPIO" pad="N14"/>
<connect gate="-P1" pin="5/GPIO" pad="N15"/>
<connect gate="-P1" pin="6/GPIO" pad="N16"/>
<connect gate="-P1" pin="7/GPIO" pad="M13"/>
<connect gate="-P2" pin="0/GPIO/RXDCAN0" pad="A16"/>
<connect gate="-P2" pin="1/GPIO/TXDCAN0" pad="G13"/>
<connect gate="-P2" pin="10/RXD0" pad="D15"/>
<connect gate="-P2" pin="11/TXD0" pad="E14"/>
<connect gate="-P2" pin="12/SCLK" pad="D14"/>
<connect gate="-P2" pin="13/MRST" pad="E13"/>
<connect gate="-P2" pin="14/MTSR" pad="C14"/>
<connect gate="-P2" pin="15/GPIO/EXI4IN/PLL_CLC.LOCK" pad="B14"/>
<connect gate="-P2" pin="2/GPIO/RXDCAN1" pad="G14"/>
<connect gate="-P2" pin="3/GPIO/TXDCAN1" pad="A15"/>
<connect gate="-P2" pin="4/GPIO" pad="F15"/>
<connect gate="-P2" pin="5/GPIO" pad="B15"/>
<connect gate="-P2" pin="6/SCL" pad="E15"/>
<connect gate="-P2" pin="7/SDA" pad="C15"/>
<connect gate="-P2" pin="8/GPIO" pad="F13"/>
<connect gate="-P2" pin="9/GPIO" pad="F14"/>
<connect gate="-P3" pin="0/GPTU.0" pad="J13"/>
<connect gate="-P3" pin="1/GPTU.1" pad="K16"/>
<connect gate="-P3" pin="10/GPIO/RXD2" pad="G16"/>
<connect gate="-P3" pin="11/GPIO/OSCBYP/TXD2" pad="E16"/>
<connect gate="-P3" pin="12/EXI5IN/HWCFG0" pad="F16"/>
<connect gate="-P3" pin="13/EXI6IN/HWCFG1" pad="G15"/>
<connect gate="-P3" pin="14/EXI7IN/HWCFG2" pad="C16"/>
<connect gate="-P3" pin="15/GPIO" pad="B16"/>
<connect gate="-P3" pin="2/GPTU.2" pad="K15"/>
<connect gate="-P3" pin="3/GPTU.3" pad="J16"/>
<connect gate="-P3" pin="4/GPTU.4" pad="H13"/>
<connect gate="-P3" pin="5/GPTU.5" pad="H14"/>
<connect gate="-P3" pin="6/GPTU.6" pad="J15"/>
<connect gate="-P3" pin="7/GPTU.7" pad="H15"/>
<connect gate="-P3" pin="8/RXD1" pad="H16"/>
<connect gate="-P3" pin="9/TXD1" pad="D16"/>
<connect gate="HS0" pin="HS" pad="N12"/>
<connect gate="HS1" pin="HS" pad="T13"/>
<connect gate="HS10" pin="HS" pad="P10"/>
<connect gate="HS11" pin="HS" pad="N10"/>
<connect gate="HS12" pin="HS" pad="T10"/>
<connect gate="HS13" pin="HS" pad="K9"/>
<connect gate="HS14" pin="HS" pad="K8"/>
<connect gate="HS15" pin="HS" pad="J7"/>
<connect gate="HS2" pin="HS" pad="R12"/>
<connect gate="HS3" pin="HS" pad="T12"/>
<connect gate="HS4" pin="HS" pad="J10"/>
<connect gate="HS5" pin="HS" pad="H10"/>
<connect gate="HS6" pin="HS" pad="P11"/>
<connect gate="HS7" pin="HS" pad="N11"/>
<connect gate="HS8" pin="HS" pad="R11"/>
<connect gate="HS9" pin="HS" pad="T11"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SAK-TC1920*" prefix="IC">
<description>&lt;b&gt;32bit Single Chip Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. TC1920_umsu_V12.pdf</description>
<gates>
<gate name="DEBUG" symbol="JTAG-OCSD-1"/>
<gate name="P3" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="AD" symbol="D31"/>
<gate name="P1" symbol="PORT8"/>
<gate name="P0" symbol="PORT8"/>
<gate name="EBU" symbol="A23"/>
<gate name="P5/TRACE" symbol="PORT16"/>
<gate name="PWR" symbol="TC1920PWR"/>
<gate name="PWR2" symbol="TC1920PWR2"/>
<gate name="G" symbol="TC1920"/>
</gates>
<devices>
<device name="" package="P-LBGA-260">
<connects>
<connect gate="AD" pin="D0" pad="L3"/>
<connect gate="AD" pin="D1" pad="L2"/>
<connect gate="AD" pin="D10" pad="H1"/>
<connect gate="AD" pin="D11" pad="H2"/>
<connect gate="AD" pin="D12" pad="H3"/>
<connect gate="AD" pin="D13" pad="G1"/>
<connect gate="AD" pin="D14" pad="G2"/>
<connect gate="AD" pin="D15" pad="G3"/>
<connect gate="AD" pin="D16" pad="H4"/>
<connect gate="AD" pin="D17" pad="G4"/>
<connect gate="AD" pin="D18" pad="E4"/>
<connect gate="AD" pin="D19" pad="F1"/>
<connect gate="AD" pin="D2" pad="K3"/>
<connect gate="AD" pin="D20" pad="F2"/>
<connect gate="AD" pin="D21" pad="F4"/>
<connect gate="AD" pin="D22" pad="F3"/>
<connect gate="AD" pin="D23" pad="E1"/>
<connect gate="AD" pin="D24" pad="E2"/>
<connect gate="AD" pin="D25" pad="E3"/>
<connect gate="AD" pin="D26" pad="D1"/>
<connect gate="AD" pin="D27" pad="C1"/>
<connect gate="AD" pin="D28" pad="D2"/>
<connect gate="AD" pin="D29" pad="D3"/>
<connect gate="AD" pin="D3" pad="K4"/>
<connect gate="AD" pin="D30" pad="C2"/>
<connect gate="AD" pin="D31" pad="B1"/>
<connect gate="AD" pin="D4" pad="L1"/>
<connect gate="AD" pin="D5" pad="K2"/>
<connect gate="AD" pin="D6" pad="K1"/>
<connect gate="AD" pin="D7" pad="J3"/>
<connect gate="AD" pin="D8" pad="J1"/>
<connect gate="AD" pin="D9" pad="J2"/>
<connect gate="DEBUG" pin="!BRKIN" pad="U15"/>
<connect gate="DEBUG" pin="!BRKOUT" pad="T14"/>
<connect gate="DEBUG" pin="!OCDSE" pad="V16"/>
<connect gate="DEBUG" pin="!TRST" pad="U17"/>
<connect gate="DEBUG" pin="TCK" pad="T16"/>
<connect gate="DEBUG" pin="TDI" pad="V17"/>
<connect gate="DEBUG" pin="TDO" pad="U16"/>
<connect gate="DEBUG" pin="TMS" pad="T15"/>
<connect gate="EBU" pin="A0" pad="V2"/>
<connect gate="EBU" pin="A1" pad="T5"/>
<connect gate="EBU" pin="A10" pad="T1"/>
<connect gate="EBU" pin="A11" pad="P3"/>
<connect gate="EBU" pin="A12" pad="R5"/>
<connect gate="EBU" pin="A13" pad="R2"/>
<connect gate="EBU" pin="A14" pad="P2"/>
<connect gate="EBU" pin="A15" pad="N3"/>
<connect gate="EBU" pin="A16" pad="R1"/>
<connect gate="EBU" pin="A17" pad="P1"/>
<connect gate="EBU" pin="A18" pad="N2"/>
<connect gate="EBU" pin="A19" pad="P4"/>
<connect gate="EBU" pin="A2" pad="V1"/>
<connect gate="EBU" pin="A20" pad="M3"/>
<connect gate="EBU" pin="A21" pad="N4"/>
<connect gate="EBU" pin="A22" pad="M4"/>
<connect gate="EBU" pin="A23" pad="N1"/>
<connect gate="EBU" pin="A3" pad="U3"/>
<connect gate="EBU" pin="A4" pad="T4"/>
<connect gate="EBU" pin="A5" pad="U2"/>
<connect gate="EBU" pin="A6" pad="T3"/>
<connect gate="EBU" pin="A7" pad="U1"/>
<connect gate="EBU" pin="A8" pad="R3"/>
<connect gate="EBU" pin="A9" pad="T2"/>
<connect gate="G" pin="/ADV" pad="R10"/>
<connect gate="G" pin="/BAA" pad="U8"/>
<connect gate="G" pin="/BC0" pad="T7"/>
<connect gate="G" pin="/BC1" pad="R6"/>
<connect gate="G" pin="/BC2" pad="V4"/>
<connect gate="G" pin="/BC3" pad="U6"/>
<connect gate="G" pin="/CAS" pad="T6"/>
<connect gate="G" pin="/CMDELAY" pad="V9"/>
<connect gate="G" pin="/CSGLB" pad="U9"/>
<connect gate="G" pin="/RAS" pad="U5"/>
<connect gate="G" pin="/RD" pad="U4"/>
<connect gate="G" pin="/SCAN_MODE" pad="K15"/>
<connect gate="G" pin="/WAIT" pad="T8"/>
<connect gate="G" pin="/WR" pad="V3"/>
<connect gate="G" pin="AI0+" pad="D13"/>
<connect gate="G" pin="AI0-" pad="A13"/>
<connect gate="G" pin="AI1+" pad="D14"/>
<connect gate="G" pin="AI1-" pad="A14"/>
<connect gate="G" pin="ALE" pad="T10"/>
<connect gate="G" pin="AO0+" pad="A15"/>
<connect gate="G" pin="AO0-" pad="B15"/>
<connect gate="G" pin="AO1+" pad="C14"/>
<connect gate="G" pin="AO1-" pad="B14"/>
<connect gate="G" pin="BFCLK0" pad="M2"/>
<connect gate="G" pin="BYPASS" pad="B17"/>
<connect gate="G" pin="CEXT" pad="A17"/>
<connect gate="G" pin="CKE" pad="U10"/>
<connect gate="G" pin="CLKOUT" pad="C17"/>
<connect gate="G" pin="CODEC_DIS" pad="C16"/>
<connect gate="G" pin="CS0" pad="R9"/>
<connect gate="G" pin="CS1" pad="R8"/>
<connect gate="G" pin="CS2" pad="R7"/>
<connect gate="G" pin="CS3" pad="V7"/>
<connect gate="G" pin="CS4" pad="V6"/>
<connect gate="G" pin="CS5" pad="V5"/>
<connect gate="G" pin="CS6" pad="U7"/>
<connect gate="G" pin="CSEMU" pad="V8"/>
<connect gate="G" pin="CSOVL" pad="T9"/>
<connect gate="G" pin="EBUCLK" pad="M1"/>
<connect gate="G" pin="HRST" pad="D16"/>
<connect gate="G" pin="MR/W" pad="V10"/>
<connect gate="G" pin="NMI" pad="A18"/>
<connect gate="G" pin="P4.0/AIN0" pad="C11"/>
<connect gate="G" pin="P4.1/AIN1" pad="A11"/>
<connect gate="G" pin="P4.2/AIN2" pad="B10"/>
<connect gate="G" pin="P4.3/AIN3" pad="A10"/>
<connect gate="G" pin="P4.4/AIN4" pad="C10"/>
<connect gate="G" pin="P4.5/AIN5" pad="A9"/>
<connect gate="G" pin="PLLCTRL_A0" pad="B8"/>
<connect gate="G" pin="PORST" pad="B18"/>
<connect gate="G" pin="TM_CTRL0" pad="B4"/>
<connect gate="G" pin="TM_CTRL1" pad="A3"/>
<connect gate="G" pin="VDDP_OSC" pad="D7"/>
<connect gate="G" pin="VDD_OSC1" pad="A7"/>
<connect gate="G" pin="VDD_OSC2" pad="C6"/>
<connect gate="G" pin="VSS_OSC" pad="B6"/>
<connect gate="G" pin="XTAL1" pad="A6"/>
<connect gate="G" pin="XTAL2" pad="B7"/>
<connect gate="G" pin="XTAL3" pad="A4"/>
<connect gate="G" pin="XTAL4" pad="B5"/>
<connect gate="P0" pin="0" pad="R18"/>
<connect gate="P0" pin="1" pad="N16"/>
<connect gate="P0" pin="2" pad="N17"/>
<connect gate="P0" pin="3" pad="P15"/>
<connect gate="P0" pin="4" pad="P18"/>
<connect gate="P0" pin="5" pad="N18"/>
<connect gate="P0" pin="6" pad="N15"/>
<connect gate="P0" pin="7" pad="M15"/>
<connect gate="P1" pin="0" pad="V18"/>
<connect gate="P1" pin="1" pad="R16"/>
<connect gate="P1" pin="2" pad="P16"/>
<connect gate="P1" pin="3" pad="T17"/>
<connect gate="P1" pin="4" pad="U18"/>
<connect gate="P1" pin="5" pad="R17"/>
<connect gate="P1" pin="6" pad="T18"/>
<connect gate="P1" pin="7" pad="P17"/>
<connect gate="P2" pin="0" pad="G18"/>
<connect gate="P2" pin="1" pad="G17"/>
<connect gate="P2" pin="10" pad="D18"/>
<connect gate="P2" pin="11" pad="C18"/>
<connect gate="P2" pin="12" pad="F16"/>
<connect gate="P2" pin="13" pad="D17"/>
<connect gate="P2" pin="14" pad="E16"/>
<connect gate="P2" pin="15" pad="F15"/>
<connect gate="P2" pin="2" pad="H16"/>
<connect gate="P2" pin="3" pad="F18"/>
<connect gate="P2" pin="4" pad="E18"/>
<connect gate="P2" pin="5" pad="F17"/>
<connect gate="P2" pin="6" pad="H15"/>
<connect gate="P2" pin="7" pad="G16"/>
<connect gate="P2" pin="8" pad="E17"/>
<connect gate="P2" pin="9" pad="G15"/>
<connect gate="P3" pin="0" pad="L15"/>
<connect gate="P3" pin="1" pad="M16"/>
<connect gate="P3" pin="10" pad="K16"/>
<connect gate="P3" pin="11" pad="J17"/>
<connect gate="P3" pin="12" pad="J15"/>
<connect gate="P3" pin="13" pad="H18"/>
<connect gate="P3" pin="14" pad="H17"/>
<connect gate="P3" pin="15" pad="J16"/>
<connect gate="P3" pin="2" pad="M17"/>
<connect gate="P3" pin="3" pad="M18"/>
<connect gate="P3" pin="4" pad="L17"/>
<connect gate="P3" pin="5" pad="L16"/>
<connect gate="P3" pin="6" pad="L18"/>
<connect gate="P3" pin="7" pad="K17"/>
<connect gate="P3" pin="8" pad="K18"/>
<connect gate="P3" pin="9" pad="J18"/>
<connect gate="P5/TRACE" pin="0" pad="V15"/>
<connect gate="P5/TRACE" pin="1" pad="U14"/>
<connect gate="P5/TRACE" pin="10" pad="V13"/>
<connect gate="P5/TRACE" pin="11" pad="U12"/>
<connect gate="P5/TRACE" pin="12" pad="T11"/>
<connect gate="P5/TRACE" pin="13" pad="V12"/>
<connect gate="P5/TRACE" pin="14" pad="U11"/>
<connect gate="P5/TRACE" pin="15" pad="V11"/>
<connect gate="P5/TRACE" pin="2" pad="T13"/>
<connect gate="P5/TRACE" pin="3" pad="R14"/>
<connect gate="P5/TRACE" pin="4" pad="V14"/>
<connect gate="P5/TRACE" pin="5" pad="R13"/>
<connect gate="P5/TRACE" pin="6" pad="U13"/>
<connect gate="P5/TRACE" pin="7" pad="T12"/>
<connect gate="P5/TRACE" pin="8" pad="R12"/>
<connect gate="P5/TRACE" pin="9" pad="R11"/>
<connect gate="PWR" pin="1V8@0" pad="A16"/>
<connect gate="PWR" pin="1V8@1" pad="B16"/>
<connect gate="PWR" pin="1V8@2" pad="B3"/>
<connect gate="PWR" pin="1V8@3" pad="C4"/>
<connect gate="PWR" pin="1V8@4" pad="D5"/>
<connect gate="PWR" pin="1V8@5" pad="J4"/>
<connect gate="PWR" pin="1V8@6" pad="L4"/>
<connect gate="PWR" pin="1V8@7" pad="R4"/>
<connect gate="PWR" pin="3V3@0" pad="G11"/>
<connect gate="PWR" pin="3V3@1" pad="G12"/>
<connect gate="PWR" pin="3V3@10" pad="M7"/>
<connect gate="PWR" pin="3V3@11" pad="M8"/>
<connect gate="PWR" pin="3V3@2" pad="G7"/>
<connect gate="PWR" pin="3V3@3" pad="G8"/>
<connect gate="PWR" pin="3V3@4" pad="H12"/>
<connect gate="PWR" pin="3V3@5" pad="H7"/>
<connect gate="PWR" pin="3V3@6" pad="L12"/>
<connect gate="PWR" pin="3V3@7" pad="L7"/>
<connect gate="PWR" pin="3V3@8" pad="M11"/>
<connect gate="PWR" pin="3V3@9" pad="M12"/>
<connect gate="PWR" pin="GND@0" pad="A1"/>
<connect gate="PWR" pin="GND@1" pad="B2"/>
<connect gate="PWR" pin="GND@10" pad="H9"/>
<connect gate="PWR" pin="GND@11" pad="J10"/>
<connect gate="PWR" pin="GND@12" pad="J11"/>
<connect gate="PWR" pin="GND@13" pad="J12"/>
<connect gate="PWR" pin="GND@14" pad="J7"/>
<connect gate="PWR" pin="GND@15" pad="J8"/>
<connect gate="PWR" pin="GND@16" pad="J9"/>
<connect gate="PWR" pin="GND@17" pad="K10"/>
<connect gate="PWR" pin="GND@18" pad="K11"/>
<connect gate="PWR" pin="GND@19" pad="K12"/>
<connect gate="PWR" pin="GND@2" pad="C3"/>
<connect gate="PWR" pin="GND@20" pad="K7"/>
<connect gate="PWR" pin="GND@21" pad="K8"/>
<connect gate="PWR" pin="GND@22" pad="K9"/>
<connect gate="PWR" pin="GND@23" pad="L10"/>
<connect gate="PWR" pin="GND@24" pad="L11"/>
<connect gate="PWR" pin="GND@25" pad="L8"/>
<connect gate="PWR" pin="GND@26" pad="L9"/>
<connect gate="PWR" pin="GND@27" pad="M10"/>
<connect gate="PWR" pin="GND@28" pad="M9"/>
<connect gate="PWR" pin="GND@3" pad="D4"/>
<connect gate="PWR" pin="GND@4" pad="D6"/>
<connect gate="PWR" pin="GND@5" pad="G10"/>
<connect gate="PWR" pin="GND@6" pad="G9"/>
<connect gate="PWR" pin="GND@7" pad="H10"/>
<connect gate="PWR" pin="GND@8" pad="H11"/>
<connect gate="PWR" pin="GND@9" pad="H8"/>
<connect gate="PWR2" pin="VAGND_ADC" pad="B11"/>
<connect gate="PWR2" pin="VAREF_ADC" pad="D11"/>
<connect gate="PWR2" pin="VDDP_ADC" pad="C12"/>
<connect gate="PWR2" pin="VDDP_COD@0" pad="E15"/>
<connect gate="PWR2" pin="VDDP_OSC@1" pad="C7"/>
<connect gate="PWR2" pin="VDDR@0" pad="A2"/>
<connect gate="PWR2" pin="VDDR@1" pad="C5"/>
<connect gate="PWR2" pin="VDD_GUARD" pad="C9"/>
<connect gate="PWR2" pin="VDD_PLL" pad="D9"/>
<connect gate="PWR2" pin="VDD_SB" pad="R15"/>
<connect gate="PWR2" pin="VGND_COD" pad="C13"/>
<connect gate="PWR2" pin="VREF_COD" pad="B13"/>
<connect gate="PWR2" pin="VSSA_ADC" pad="A12"/>
<connect gate="PWR2" pin="VSSA_COD@0" pad="D15"/>
<connect gate="PWR2" pin="VSSP_ADC@0" pad="B12"/>
<connect gate="PWR2" pin="VSSP_ADC@1" pad="D12"/>
<connect gate="PWR2" pin="VSSP_ADC@2" pad="D10"/>
<connect gate="PWR2" pin="VSSP_COD@0" pad="C15"/>
<connect gate="PWR2" pin="VSSP_OSC@0" pad="D8"/>
<connect gate="PWR2" pin="VSSP_OSC@1" pad="A5"/>
<connect gate="PWR2" pin="VSS_GUARD@1" pad="A8"/>
<connect gate="PWR2" pin="VSS_GUARD@2" pad="C8"/>
<connect gate="PWR2" pin="VSS_PLL" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC-10" prefix="IC">
<description>&lt;b&gt;+ Obsolete +&lt;/b&gt; TC10 GP TriCore 32bit  Microcontroller+ DSP&lt;p&gt;
Source: http://www.infineon.com ..</description>
<gates>
<gate name="G" symbol="TC10"/>
<gate name="G$2" symbol="VSSE_VDD"/>
<gate name="G$3" symbol="VSSE_VDD"/>
<gate name="G$4" symbol="VSSE_VDD"/>
<gate name="G$5" symbol="VSSE_VDD"/>
<gate name="G$6" symbol="VSSE_VDD"/>
<gate name="G$7" symbol="VSSE_VDD"/>
<gate name="G$8" symbol="VSSE_VDD"/>
<gate name="G$9" symbol="VSSE_VDD"/>
<gate name="G$10" symbol="VSSE_VDD"/>
<gate name="G$11" symbol="VSSE_VDD"/>
<gate name="G$12" symbol="VSSE_VDD"/>
<gate name="G$13" symbol="VSSE_VDD"/>
<gate name="G$14" symbol="VSSE_VDD"/>
<gate name="G$15" symbol="VSSE_VDD"/>
<gate name="G$16" symbol="VSSE_VDD"/>
<gate name="G$17" symbol="VSSE_VDD"/>
<gate name="G$18" symbol="VSSE_VDD"/>
<gate name="G$19" symbol="VSSE_VDD"/>
<gate name="G$20" symbol="VSSE_VDD"/>
<gate name="G$21" symbol="VSS_VDD"/>
<gate name="G$22" symbol="VSS_VDD"/>
<gate name="G$23" symbol="VSS_VDD"/>
<gate name="G$24" symbol="VSS_VDD"/>
<gate name="G$25" symbol="VSS_VDD"/>
<gate name="G$26" symbol="VSS_VDD"/>
<gate name="G$27" symbol="VSS_VDD"/>
<gate name="G$28" symbol="VSSP_VDD"/>
<gate name="G$1" symbol="VSSE_VDD"/>
<gate name="G$29" symbol="VSS_VDD"/>
</gates>
<devices>
<device name="" package="FQFP208-2">
<connects>
<connect gate="G" pin="(CHIPZ)" pad="54"/>
<connect gate="G" pin="/BREQ" pad="105"/>
<connect gate="G" pin="/CAS" pad="153"/>
<connect gate="G" pin="/CODE" pad="152"/>
<connect gate="G" pin="/CSFM" pad="161"/>
<connect gate="G" pin="/CSFPI" pad="157"/>
<connect gate="G" pin="/CSOL" pad="160"/>
<connect gate="G" pin="/HLDA" pad="104"/>
<connect gate="G" pin="/HOLD" pad="103"/>
<connect gate="G" pin="/HRST" pad="51"/>
<connect gate="G" pin="/POR" pad="52"/>
<connect gate="G" pin="/RAS" pad="154"/>
<connect gate="G" pin="/RD" pad="156"/>
<connect gate="G" pin="/WAIT" pad="158"/>
<connect gate="G" pin="/WR" pad="155"/>
<connect gate="G" pin="A0" pad="177"/>
<connect gate="G" pin="A1" pad="178"/>
<connect gate="G" pin="A10" pad="189"/>
<connect gate="G" pin="A11" pad="190"/>
<connect gate="G" pin="A12" pad="191"/>
<connect gate="G" pin="A13" pad="196"/>
<connect gate="G" pin="A14" pad="197"/>
<connect gate="G" pin="A15" pad="198"/>
<connect gate="G" pin="A16" pad="199"/>
<connect gate="G" pin="A17" pad="200"/>
<connect gate="G" pin="A18" pad="201"/>
<connect gate="G" pin="A19" pad="204"/>
<connect gate="G" pin="A2" pad="179"/>
<connect gate="G" pin="A20" pad="205"/>
<connect gate="G" pin="A21" pad="206"/>
<connect gate="G" pin="A22" pad="207"/>
<connect gate="G" pin="A23" pad="208"/>
<connect gate="G" pin="A3" pad="180"/>
<connect gate="G" pin="A4" pad="181"/>
<connect gate="G" pin="A5" pad="184"/>
<connect gate="G" pin="A6" pad="185"/>
<connect gate="G" pin="A7" pad="186"/>
<connect gate="G" pin="A8" pad="187"/>
<connect gate="G" pin="A9" pad="188"/>
<connect gate="G" pin="AD0" pad="149"/>
<connect gate="G" pin="AD1" pad="148"/>
<connect gate="G" pin="AD10" pad="135"/>
<connect gate="G" pin="AD11" pad="134"/>
<connect gate="G" pin="AD12" pad="133"/>
<connect gate="G" pin="AD13" pad="132"/>
<connect gate="G" pin="AD14" pad="129"/>
<connect gate="G" pin="AD15" pad="128"/>
<connect gate="G" pin="AD16" pad="127"/>
<connect gate="G" pin="AD17" pad="126"/>
<connect gate="G" pin="AD18" pad="125"/>
<connect gate="G" pin="AD19" pad="124"/>
<connect gate="G" pin="AD2" pad="147"/>
<connect gate="G" pin="AD20" pad="123"/>
<connect gate="G" pin="AD21" pad="122"/>
<connect gate="G" pin="AD22" pad="117"/>
<connect gate="G" pin="AD23" pad="116"/>
<connect gate="G" pin="AD24" pad="115"/>
<connect gate="G" pin="AD25" pad="114"/>
<connect gate="G" pin="AD26" pad="113"/>
<connect gate="G" pin="AD27" pad="112"/>
<connect gate="G" pin="AD28" pad="109"/>
<connect gate="G" pin="AD29" pad="108"/>
<connect gate="G" pin="AD3" pad="146"/>
<connect gate="G" pin="AD30" pad="107"/>
<connect gate="G" pin="AD31" pad="106"/>
<connect gate="G" pin="AD4" pad="145"/>
<connect gate="G" pin="AD5" pad="144"/>
<connect gate="G" pin="AD6" pad="139"/>
<connect gate="G" pin="AD7" pad="138"/>
<connect gate="G" pin="AD8" pad="137"/>
<connect gate="G" pin="AD9" pad="136"/>
<connect gate="G" pin="ALE" pad="159"/>
<connect gate="G" pin="BC0" pad="169"/>
<connect gate="G" pin="BC1" pad="174"/>
<connect gate="G" pin="BC2" pad="175"/>
<connect gate="G" pin="BC3" pad="176"/>
<connect gate="G" pin="BRKPT0" pad="60"/>
<connect gate="G" pin="BRKPT1" pad="57"/>
<connect gate="G" pin="BRKPT2" pad="56"/>
<connect gate="G" pin="BRK_OUT" pad="55"/>
<connect gate="G" pin="BYPASS" pad="84"/>
<connect gate="G" pin="CLKS@0" pad="11"/>
<connect gate="G" pin="CLKS@1" pad="12"/>
<connect gate="G" pin="CLKS@2" pad="13"/>
<connect gate="G" pin="CS0" pad="165"/>
<connect gate="G" pin="CS1" pad="166"/>
<connect gate="G" pin="CS2" pad="167"/>
<connect gate="G" pin="CS3" pad="168"/>
<connect gate="G" pin="EBUC" pad="163"/>
<connect gate="G" pin="IND_PC0" pad="74"/>
<connect gate="G" pin="IND_PC1" pad="75"/>
<connect gate="G" pin="IND_PC2" pad="76"/>
<connect gate="G" pin="IND_PC3" pad="77"/>
<connect gate="G" pin="IND_PC4" pad="80"/>
<connect gate="G" pin="IND_PC5" pad="81"/>
<connect gate="G" pin="IND_PC6" pad="82"/>
<connect gate="G" pin="IND_PC7" pad="83"/>
<connect gate="G" pin="NC@0" pad="85"/>
<connect gate="G" pin="NC@1" pad="86"/>
<connect gate="G" pin="NC@2" pad="87"/>
<connect gate="G" pin="NMI" pad="50"/>
<connect gate="G" pin="OCDS_E" pad="53"/>
<connect gate="G" pin="P0.0" pad="18"/>
<connect gate="G" pin="P0.1" pad="19"/>
<connect gate="G" pin="P0.2" pad="20"/>
<connect gate="G" pin="P0.3" pad="21"/>
<connect gate="G" pin="P0.4" pad="22"/>
<connect gate="G" pin="P0.5" pad="23"/>
<connect gate="G" pin="P0.6" pad="24"/>
<connect gate="G" pin="P0.7" pad="25"/>
<connect gate="G" pin="P1.0" pad="28"/>
<connect gate="G" pin="P1.1" pad="29"/>
<connect gate="G" pin="P1.2" pad="30"/>
<connect gate="G" pin="P1.3" pad="31"/>
<connect gate="G" pin="P1.4" pad="32"/>
<connect gate="G" pin="P1.5" pad="33"/>
<connect gate="G" pin="P1.6" pad="34"/>
<connect gate="G" pin="P1.7" pad="35"/>
<connect gate="G" pin="P2.0" pad="40"/>
<connect gate="G" pin="P2.1" pad="41"/>
<connect gate="G" pin="P2.2" pad="42"/>
<connect gate="G" pin="P2.3" pad="43"/>
<connect gate="G" pin="P2.4" pad="44"/>
<connect gate="G" pin="P2.5" pad="45"/>
<connect gate="G" pin="P2.6" pad="48"/>
<connect gate="G" pin="P2.7" pad="49"/>
<connect gate="G" pin="PCP_PC0" pad="102"/>
<connect gate="G" pin="PCP_PC1" pad="101"/>
<connect gate="G" pin="PCP_PC2" pad="100"/>
<connect gate="G" pin="PCP_PC3" pad="97"/>
<connect gate="G" pin="PCP_PC4" pad="96"/>
<connect gate="G" pin="PCP_PC5" pad="95"/>
<connect gate="G" pin="PCP_PC6" pad="94"/>
<connect gate="G" pin="PCP_PC7" pad="93"/>
<connect gate="G" pin="PCP_PC8" pad="92"/>
<connect gate="G" pin="SCAN@0" pad="8"/>
<connect gate="G" pin="SCAN@1" pad="9"/>
<connect gate="G" pin="STATUS0" pad="65"/>
<connect gate="G" pin="STATUS1" pad="64"/>
<connect gate="G" pin="STATUS2" pad="63"/>
<connect gate="G" pin="STATUS3" pad="62"/>
<connect gate="G" pin="STATUS4" pad="61"/>
<connect gate="G" pin="TCK" pad="2"/>
<connect gate="G" pin="TDI" pad="4"/>
<connect gate="G" pin="TDO" pad="5"/>
<connect gate="G" pin="TMS" pad="3"/>
<connect gate="G" pin="TRST" pad="1"/>
<connect gate="G" pin="VCOS" pad="10"/>
<connect gate="G" pin="XTAL1" pad="71"/>
<connect gate="G" pin="XTAL2" pad="70"/>
<connect gate="G$1" pin="VDDE" pad="6"/>
<connect gate="G$1" pin="VSSE" pad="7"/>
<connect gate="G$10" pin="VDDE" pad="118"/>
<connect gate="G$10" pin="VSSE" pad="119"/>
<connect gate="G$11" pin="VDDE" pad="130"/>
<connect gate="G$11" pin="VSSE" pad="131"/>
<connect gate="G$12" pin="VDDE" pad="140"/>
<connect gate="G$12" pin="VSSE" pad="141"/>
<connect gate="G$13" pin="VDDE" pad="150"/>
<connect gate="G$13" pin="VSSE" pad="151"/>
<connect gate="G$14" pin="VDDE" pad="162"/>
<connect gate="G$14" pin="VSSE" pad="164"/>
<connect gate="G$15" pin="VDDE" pad="170"/>
<connect gate="G$15" pin="VSSE" pad="171"/>
<connect gate="G$16" pin="VDDE" pad="182"/>
<connect gate="G$16" pin="VSSE" pad="183"/>
<connect gate="G$17" pin="VDDE" pad="202"/>
<connect gate="G$17" pin="VSSE" pad="203"/>
<connect gate="G$18" pin="VDDE" pad="46"/>
<connect gate="G$18" pin="VSSE" pad="47"/>
<connect gate="G$19" pin="VDDE" pad="58"/>
<connect gate="G$19" pin="VSSE" pad="59"/>
<connect gate="G$2" pin="VDDE" pad="14"/>
<connect gate="G$2" pin="VSSE" pad="15"/>
<connect gate="G$20" pin="VDDE" pad="192"/>
<connect gate="G$20" pin="VSSE" pad="193"/>
<connect gate="G$21" pin="VDD" pad="17"/>
<connect gate="G$21" pin="VSS" pad="16"/>
<connect gate="G$22" pin="VDD" pad="39"/>
<connect gate="G$22" pin="VSS" pad="38"/>
<connect gate="G$23" pin="VDD" pad="69"/>
<connect gate="G$23" pin="VSS" pad="68"/>
<connect gate="G$24" pin="VDD" pad="91"/>
<connect gate="G$24" pin="VSS" pad="90"/>
<connect gate="G$25" pin="VDD" pad="121"/>
<connect gate="G$25" pin="VSS" pad="120"/>
<connect gate="G$26" pin="VDD" pad="143"/>
<connect gate="G$26" pin="VSS" pad="142"/>
<connect gate="G$27" pin="VDD" pad="173"/>
<connect gate="G$27" pin="VSS" pad="172"/>
<connect gate="G$28" pin="VDDP" pad="73"/>
<connect gate="G$28" pin="VSSP" pad="72"/>
<connect gate="G$29" pin="VDD" pad="195"/>
<connect gate="G$29" pin="VSS" pad="194"/>
<connect gate="G$3" pin="VDDE" pad="26"/>
<connect gate="G$3" pin="VSSE" pad="27"/>
<connect gate="G$4" pin="VDDE" pad="36"/>
<connect gate="G$4" pin="VSSE" pad="37"/>
<connect gate="G$5" pin="VDDE" pad="66"/>
<connect gate="G$5" pin="VSSE" pad="67"/>
<connect gate="G$6" pin="VDDE" pad="78"/>
<connect gate="G$6" pin="VSSE" pad="79"/>
<connect gate="G$7" pin="VDDE" pad="88"/>
<connect gate="G$7" pin="VSSE" pad="89"/>
<connect gate="G$8" pin="VDDE" pad="98"/>
<connect gate="G$8" pin="VSSE" pad="99"/>
<connect gate="G$9" pin="VDDE" pad="110"/>
<connect gate="G$9" pin="VSSE" pad="111"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC10" prefix="IC">
<description>&lt;b&gt;+ Obsolete +&lt;/b&gt; TC10 GP TriCore 32bit  Microcontroller+ DSP&lt;p&gt;
Source: http://www.infineon.com ..</description>
<gates>
<gate name="G" symbol="TC10"/>
<gate name="G$2" symbol="VSSE_VDD"/>
<gate name="G$3" symbol="VSSE_VDD"/>
<gate name="G$4" symbol="VSSE_VDD"/>
<gate name="G$5" symbol="VSSE_VDD"/>
<gate name="G$6" symbol="VSSE_VDD"/>
<gate name="G$7" symbol="VSSE_VDD"/>
<gate name="G$8" symbol="VSSE_VDD"/>
<gate name="G$9" symbol="VSSE_VDD"/>
<gate name="G$10" symbol="VSSE_VDD"/>
<gate name="G$11" symbol="VSSE_VDD"/>
<gate name="G$12" symbol="VSSE_VDD"/>
<gate name="G$13" symbol="VSSE_VDD"/>
<gate name="G$14" symbol="VSSE_VDD"/>
<gate name="G$15" symbol="VSSE_VDD"/>
<gate name="G$16" symbol="VSSE_VDD"/>
<gate name="G$17" symbol="VSSE_VDD"/>
<gate name="G$18" symbol="VSSE_VDD"/>
<gate name="G$19" symbol="VSSE_VDD"/>
<gate name="G$20" symbol="VSSE_VDD"/>
<gate name="G$21" symbol="VSS_VDD"/>
<gate name="G$22" symbol="VSS_VDD"/>
<gate name="G$23" symbol="VSS_VDD"/>
<gate name="G$24" symbol="VSS_VDD"/>
<gate name="G$25" symbol="VSS_VDD"/>
<gate name="G$26" symbol="VSS_VDD"/>
<gate name="G$27" symbol="VSS_VDD"/>
<gate name="G$28" symbol="VSSP_VDD"/>
<gate name="G$1" symbol="VSSE_VDD"/>
<gate name="G$29" symbol="VSS_VDD"/>
</gates>
<devices>
<device name="" package="FQFP208-2">
<connects>
<connect gate="G" pin="(CHIPZ)" pad="54"/>
<connect gate="G" pin="/BREQ" pad="105"/>
<connect gate="G" pin="/CAS" pad="153"/>
<connect gate="G" pin="/CODE" pad="152"/>
<connect gate="G" pin="/CSFM" pad="161"/>
<connect gate="G" pin="/CSFPI" pad="157"/>
<connect gate="G" pin="/CSOL" pad="160"/>
<connect gate="G" pin="/HLDA" pad="104"/>
<connect gate="G" pin="/HOLD" pad="103"/>
<connect gate="G" pin="/HRST" pad="51"/>
<connect gate="G" pin="/POR" pad="52"/>
<connect gate="G" pin="/RAS" pad="154"/>
<connect gate="G" pin="/RD" pad="156"/>
<connect gate="G" pin="/WAIT" pad="158"/>
<connect gate="G" pin="/WR" pad="155"/>
<connect gate="G" pin="A0" pad="177"/>
<connect gate="G" pin="A1" pad="178"/>
<connect gate="G" pin="A10" pad="189"/>
<connect gate="G" pin="A11" pad="190"/>
<connect gate="G" pin="A12" pad="191"/>
<connect gate="G" pin="A13" pad="196"/>
<connect gate="G" pin="A14" pad="197"/>
<connect gate="G" pin="A15" pad="198"/>
<connect gate="G" pin="A16" pad="199"/>
<connect gate="G" pin="A17" pad="200"/>
<connect gate="G" pin="A18" pad="201"/>
<connect gate="G" pin="A19" pad="204"/>
<connect gate="G" pin="A2" pad="179"/>
<connect gate="G" pin="A20" pad="205"/>
<connect gate="G" pin="A21" pad="206"/>
<connect gate="G" pin="A22" pad="207"/>
<connect gate="G" pin="A23" pad="208"/>
<connect gate="G" pin="A3" pad="180"/>
<connect gate="G" pin="A4" pad="181"/>
<connect gate="G" pin="A5" pad="184"/>
<connect gate="G" pin="A6" pad="185"/>
<connect gate="G" pin="A7" pad="186"/>
<connect gate="G" pin="A8" pad="187"/>
<connect gate="G" pin="A9" pad="188"/>
<connect gate="G" pin="AD0" pad="149"/>
<connect gate="G" pin="AD1" pad="148"/>
<connect gate="G" pin="AD10" pad="135"/>
<connect gate="G" pin="AD11" pad="134"/>
<connect gate="G" pin="AD12" pad="133"/>
<connect gate="G" pin="AD13" pad="132"/>
<connect gate="G" pin="AD14" pad="129"/>
<connect gate="G" pin="AD15" pad="128"/>
<connect gate="G" pin="AD16" pad="127"/>
<connect gate="G" pin="AD17" pad="126"/>
<connect gate="G" pin="AD18" pad="125"/>
<connect gate="G" pin="AD19" pad="124"/>
<connect gate="G" pin="AD2" pad="147"/>
<connect gate="G" pin="AD20" pad="123"/>
<connect gate="G" pin="AD21" pad="122"/>
<connect gate="G" pin="AD22" pad="117"/>
<connect gate="G" pin="AD23" pad="116"/>
<connect gate="G" pin="AD24" pad="115"/>
<connect gate="G" pin="AD25" pad="114"/>
<connect gate="G" pin="AD26" pad="113"/>
<connect gate="G" pin="AD27" pad="112"/>
<connect gate="G" pin="AD28" pad="109"/>
<connect gate="G" pin="AD29" pad="108"/>
<connect gate="G" pin="AD3" pad="146"/>
<connect gate="G" pin="AD30" pad="107"/>
<connect gate="G" pin="AD31" pad="106"/>
<connect gate="G" pin="AD4" pad="145"/>
<connect gate="G" pin="AD5" pad="144"/>
<connect gate="G" pin="AD6" pad="139"/>
<connect gate="G" pin="AD7" pad="138"/>
<connect gate="G" pin="AD8" pad="137"/>
<connect gate="G" pin="AD9" pad="136"/>
<connect gate="G" pin="ALE" pad="159"/>
<connect gate="G" pin="BC0" pad="169"/>
<connect gate="G" pin="BC1" pad="174"/>
<connect gate="G" pin="BC2" pad="175"/>
<connect gate="G" pin="BC3" pad="176"/>
<connect gate="G" pin="BRKPT0" pad="60"/>
<connect gate="G" pin="BRKPT1" pad="57"/>
<connect gate="G" pin="BRKPT2" pad="56"/>
<connect gate="G" pin="BRK_OUT" pad="55"/>
<connect gate="G" pin="BYPASS" pad="84"/>
<connect gate="G" pin="CLKS@0" pad="11"/>
<connect gate="G" pin="CLKS@1" pad="12"/>
<connect gate="G" pin="CLKS@2" pad="13"/>
<connect gate="G" pin="CS0" pad="165"/>
<connect gate="G" pin="CS1" pad="166"/>
<connect gate="G" pin="CS2" pad="167"/>
<connect gate="G" pin="CS3" pad="168"/>
<connect gate="G" pin="EBUC" pad="163"/>
<connect gate="G" pin="IND_PC0" pad="74"/>
<connect gate="G" pin="IND_PC1" pad="75"/>
<connect gate="G" pin="IND_PC2" pad="76"/>
<connect gate="G" pin="IND_PC3" pad="77"/>
<connect gate="G" pin="IND_PC4" pad="80"/>
<connect gate="G" pin="IND_PC5" pad="81"/>
<connect gate="G" pin="IND_PC6" pad="82"/>
<connect gate="G" pin="IND_PC7" pad="83"/>
<connect gate="G" pin="NC@0" pad="85"/>
<connect gate="G" pin="NC@1" pad="86"/>
<connect gate="G" pin="NC@2" pad="87"/>
<connect gate="G" pin="NMI" pad="50"/>
<connect gate="G" pin="OCDS_E" pad="53"/>
<connect gate="G" pin="P0.0" pad="18"/>
<connect gate="G" pin="P0.1" pad="19"/>
<connect gate="G" pin="P0.2" pad="20"/>
<connect gate="G" pin="P0.3" pad="21"/>
<connect gate="G" pin="P0.4" pad="22"/>
<connect gate="G" pin="P0.5" pad="23"/>
<connect gate="G" pin="P0.6" pad="24"/>
<connect gate="G" pin="P0.7" pad="25"/>
<connect gate="G" pin="P1.0" pad="28"/>
<connect gate="G" pin="P1.1" pad="29"/>
<connect gate="G" pin="P1.2" pad="30"/>
<connect gate="G" pin="P1.3" pad="31"/>
<connect gate="G" pin="P1.4" pad="32"/>
<connect gate="G" pin="P1.5" pad="33"/>
<connect gate="G" pin="P1.6" pad="34"/>
<connect gate="G" pin="P1.7" pad="35"/>
<connect gate="G" pin="P2.0" pad="40"/>
<connect gate="G" pin="P2.1" pad="41"/>
<connect gate="G" pin="P2.2" pad="42"/>
<connect gate="G" pin="P2.3" pad="43"/>
<connect gate="G" pin="P2.4" pad="44"/>
<connect gate="G" pin="P2.5" pad="45"/>
<connect gate="G" pin="P2.6" pad="48"/>
<connect gate="G" pin="P2.7" pad="49"/>
<connect gate="G" pin="PCP_PC0" pad="102"/>
<connect gate="G" pin="PCP_PC1" pad="101"/>
<connect gate="G" pin="PCP_PC2" pad="100"/>
<connect gate="G" pin="PCP_PC3" pad="97"/>
<connect gate="G" pin="PCP_PC4" pad="96"/>
<connect gate="G" pin="PCP_PC5" pad="95"/>
<connect gate="G" pin="PCP_PC6" pad="94"/>
<connect gate="G" pin="PCP_PC7" pad="93"/>
<connect gate="G" pin="PCP_PC8" pad="92"/>
<connect gate="G" pin="SCAN@0" pad="8"/>
<connect gate="G" pin="SCAN@1" pad="9"/>
<connect gate="G" pin="STATUS0" pad="65"/>
<connect gate="G" pin="STATUS1" pad="64"/>
<connect gate="G" pin="STATUS2" pad="63"/>
<connect gate="G" pin="STATUS3" pad="62"/>
<connect gate="G" pin="STATUS4" pad="61"/>
<connect gate="G" pin="TCK" pad="2"/>
<connect gate="G" pin="TDI" pad="4"/>
<connect gate="G" pin="TDO" pad="5"/>
<connect gate="G" pin="TMS" pad="3"/>
<connect gate="G" pin="TRST" pad="1"/>
<connect gate="G" pin="VCOS" pad="10"/>
<connect gate="G" pin="XTAL1" pad="71"/>
<connect gate="G" pin="XTAL2" pad="70"/>
<connect gate="G$1" pin="VDDE" pad="6"/>
<connect gate="G$1" pin="VSSE" pad="7"/>
<connect gate="G$10" pin="VDDE" pad="118"/>
<connect gate="G$10" pin="VSSE" pad="119"/>
<connect gate="G$11" pin="VDDE" pad="130"/>
<connect gate="G$11" pin="VSSE" pad="131"/>
<connect gate="G$12" pin="VDDE" pad="140"/>
<connect gate="G$12" pin="VSSE" pad="141"/>
<connect gate="G$13" pin="VDDE" pad="150"/>
<connect gate="G$13" pin="VSSE" pad="151"/>
<connect gate="G$14" pin="VDDE" pad="162"/>
<connect gate="G$14" pin="VSSE" pad="164"/>
<connect gate="G$15" pin="VDDE" pad="170"/>
<connect gate="G$15" pin="VSSE" pad="171"/>
<connect gate="G$16" pin="VDDE" pad="182"/>
<connect gate="G$16" pin="VSSE" pad="183"/>
<connect gate="G$17" pin="VDDE" pad="202"/>
<connect gate="G$17" pin="VSSE" pad="203"/>
<connect gate="G$18" pin="VDDE" pad="46"/>
<connect gate="G$18" pin="VSSE" pad="47"/>
<connect gate="G$19" pin="VDDE" pad="58"/>
<connect gate="G$19" pin="VSSE" pad="59"/>
<connect gate="G$2" pin="VDDE" pad="14"/>
<connect gate="G$2" pin="VSSE" pad="15"/>
<connect gate="G$20" pin="VDDE" pad="192"/>
<connect gate="G$20" pin="VSSE" pad="193"/>
<connect gate="G$21" pin="VDD" pad="17"/>
<connect gate="G$21" pin="VSS" pad="16"/>
<connect gate="G$22" pin="VDD" pad="39"/>
<connect gate="G$22" pin="VSS" pad="38"/>
<connect gate="G$23" pin="VDD" pad="69"/>
<connect gate="G$23" pin="VSS" pad="68"/>
<connect gate="G$24" pin="VDD" pad="91"/>
<connect gate="G$24" pin="VSS" pad="90"/>
<connect gate="G$25" pin="VDD" pad="121"/>
<connect gate="G$25" pin="VSS" pad="120"/>
<connect gate="G$26" pin="VDD" pad="143"/>
<connect gate="G$26" pin="VSS" pad="142"/>
<connect gate="G$27" pin="VDD" pad="173"/>
<connect gate="G$27" pin="VSS" pad="172"/>
<connect gate="G$28" pin="VDDP" pad="73"/>
<connect gate="G$28" pin="VSSP" pad="72"/>
<connect gate="G$29" pin="VDD" pad="195"/>
<connect gate="G$29" pin="VSS" pad="194"/>
<connect gate="G$3" pin="VDDE" pad="26"/>
<connect gate="G$3" pin="VSSE" pad="27"/>
<connect gate="G$4" pin="VDDE" pad="36"/>
<connect gate="G$4" pin="VSSE" pad="37"/>
<connect gate="G$5" pin="VDDE" pad="66"/>
<connect gate="G$5" pin="VSSE" pad="67"/>
<connect gate="G$6" pin="VDDE" pad="78"/>
<connect gate="G$6" pin="VSSE" pad="79"/>
<connect gate="G$7" pin="VDDE" pad="88"/>
<connect gate="G$7" pin="VSSE" pad="89"/>
<connect gate="G$8" pin="VDDE" pad="98"/>
<connect gate="G$8" pin="VSSE" pad="99"/>
<connect gate="G$9" pin="VDDE" pad="110"/>
<connect gate="G$9" pin="VSSE" pad="111"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC11IB" prefix="IC">
<description>&lt;b&gt;32-Bit Single-Chip Microcontroller TriCore Family&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. TC11IB_DS_v24.pdf</description>
<gates>
<gate name="-C" symbol="TC11IB"/>
<gate name="-PCI" symbol="PCI"/>
<gate name="-AD" symbol="AD31"/>
<gate name="-JTAG" symbol="ODCS/JTAG"/>
<gate name="-P0" symbol="PORT16"/>
<gate name="-P1" symbol="PORT16"/>
<gate name="-P2" symbol="PORT16"/>
<gate name="-P3" symbol="PORT16"/>
<gate name="-P4" symbol="PORT16"/>
<gate name="-P5" symbol="PORT16"/>
<gate name="-P_AD" symbol="AD31"/>
<gate name="-A" symbol="A23"/>
<gate name="-VSS1" symbol="VSS"/>
<gate name="-VSS2" symbol="VSS"/>
<gate name="-VSS3" symbol="VSS"/>
<gate name="-VSS4" symbol="VSS"/>
<gate name="-VSS5" symbol="VSS"/>
<gate name="-VSS6" symbol="VSS"/>
<gate name="-VSS7" symbol="VSS"/>
<gate name="-VSS8" symbol="VSS"/>
<gate name="-VSS9" symbol="VSS"/>
<gate name="-VSS10" symbol="VSS"/>
<gate name="-VSS11" symbol="VSS"/>
<gate name="-VSS12" symbol="VSS"/>
<gate name="-VSS13" symbol="VSS"/>
<gate name="-VSS14" symbol="VSS"/>
<gate name="-VSS15" symbol="VSS"/>
<gate name="-VSS16" symbol="VSS"/>
<gate name="-VSS17" symbol="VSS"/>
<gate name="-VSS18" symbol="VSS"/>
<gate name="-VSS19" symbol="VSS"/>
<gate name="-VSS20" symbol="VSS"/>
<gate name="-VSS21" symbol="VSS"/>
<gate name="-VSS22" symbol="VSS"/>
<gate name="-VSS23" symbol="VSS"/>
<gate name="-VSS24" symbol="VSS"/>
<gate name="-VSS25" symbol="VSS"/>
<gate name="-VSS26" symbol="VSS"/>
<gate name="-VSS27" symbol="VSS"/>
<gate name="-VSS28" symbol="VSS"/>
<gate name="-VSS29" symbol="VSS"/>
<gate name="-VSS30" symbol="VSS"/>
<gate name="-VSS31" symbol="VSS"/>
<gate name="-VSS32" symbol="VSS"/>
<gate name="-VSS33" symbol="VSS"/>
<gate name="-VSS34" symbol="VSS"/>
<gate name="-VSS35" symbol="VSS"/>
<gate name="-VSS36" symbol="VSS"/>
<gate name="-VSS37" symbol="VSS"/>
<gate name="-VSS38" symbol="VSS"/>
<gate name="-VSS39" symbol="VSS"/>
<gate name="-VSS40" symbol="VSS"/>
<gate name="-VSS41" symbol="VSS"/>
<gate name="-VSS42" symbol="VSS"/>
<gate name="-VSS43" symbol="VSS"/>
<gate name="-VSS44" symbol="VSS"/>
<gate name="-VSS45" symbol="VSS"/>
<gate name="-VSS46" symbol="VSS"/>
<gate name="-VSS47" symbol="VSS"/>
<gate name="-VSS48" symbol="VSS"/>
<gate name="-VSS49" symbol="VSS"/>
<gate name="-VSS50" symbol="VSS"/>
<gate name="-VSS51" symbol="VSS"/>
<gate name="-VSS52" symbol="VSS"/>
<gate name="VDDP1" symbol="VDDP"/>
<gate name="VDDP2" symbol="VDDP"/>
<gate name="VDDP3" symbol="VDDP"/>
<gate name="VDDP4" symbol="VDDP"/>
<gate name="VDDP5" symbol="VDDP"/>
<gate name="VDDP6" symbol="VDDP"/>
<gate name="VDDP7" symbol="VDDP"/>
<gate name="VDDP8" symbol="VDDP"/>
<gate name="VDDP9" symbol="VDDP"/>
<gate name="VDDP10" symbol="VDDP"/>
<gate name="VDDP11" symbol="VDDP"/>
<gate name="VDDP12" symbol="VDDP"/>
<gate name="VDDP13" symbol="VDDP"/>
<gate name="VDDP14" symbol="VDDP"/>
<gate name="VDDP15" symbol="VDDP"/>
<gate name="VDDP16" symbol="VDDP"/>
<gate name="VDDP17" symbol="VDDP"/>
<gate name="VDDP18" symbol="VDDP"/>
<gate name="VDDP19" symbol="VDDP"/>
<gate name="VDDP20" symbol="VDDP"/>
<gate name="VDD1" symbol="VDD"/>
<gate name="VDD2" symbol="VDD"/>
<gate name="VDD3" symbol="VDD"/>
<gate name="VDD4" symbol="VDD"/>
<gate name="VDD5" symbol="VDD"/>
<gate name="VDD6" symbol="VDD"/>
<gate name="VDD7" symbol="VDD"/>
<gate name="VDD8" symbol="VDD"/>
<gate name="VDD9" symbol="VDD"/>
<gate name="VDD10" symbol="VDD"/>
<gate name="VDD11" symbol="VDD"/>
<gate name="VDD12" symbol="VDD"/>
<gate name="VDD13" symbol="VDD"/>
<gate name="VDD14" symbol="VDD"/>
<gate name="VDD15" symbol="VDD"/>
<gate name="VDD16" symbol="VDD"/>
<gate name="VDD17" symbol="VDD"/>
<gate name="VDD18" symbol="VDD"/>
<gate name="VDD19" symbol="VDD"/>
<gate name="VDD20" symbol="VDD"/>
<gate name="VDD21" symbol="VDD"/>
</gates>
<devices>
<device name="" package="P-BGA-388-2">
<connects>
<connect gate="-A" pin="A0" pad="AA26"/>
<connect gate="-A" pin="A1" pad="V24"/>
<connect gate="-A" pin="A10" pad="V26"/>
<connect gate="-A" pin="A11" pad="U25"/>
<connect gate="-A" pin="A12" pad="U24"/>
<connect gate="-A" pin="A13" pad="U26"/>
<connect gate="-A" pin="A14" pad="T26"/>
<connect gate="-A" pin="A15" pad="T25"/>
<connect gate="-A" pin="A16" pad="T24"/>
<connect gate="-A" pin="A17" pad="R23"/>
<connect gate="-A" pin="A18" pad="R24"/>
<connect gate="-A" pin="A19" pad="R25"/>
<connect gate="-A" pin="A2" pad="W24"/>
<connect gate="-A" pin="A20" pad="A24"/>
<connect gate="-A" pin="A21" pad="B23"/>
<connect gate="-A" pin="A22" pad="C23"/>
<connect gate="-A" pin="A23" pad="D22"/>
<connect gate="-A" pin="A3" pad="Y24"/>
<connect gate="-A" pin="A4" pad="Y25"/>
<connect gate="-A" pin="A5" pad="AA25"/>
<connect gate="-A" pin="A6" pad="Y26"/>
<connect gate="-A" pin="A7" pad="W25"/>
<connect gate="-A" pin="A8" pad="W26"/>
<connect gate="-A" pin="A9" pad="V25"/>
<connect gate="-AD" pin="AD0" pad="L25"/>
<connect gate="-AD" pin="AD1" pad="L24"/>
<connect gate="-AD" pin="AD10" pad="J25"/>
<connect gate="-AD" pin="AD11" pad="H26"/>
<connect gate="-AD" pin="AD12" pad="H25"/>
<connect gate="-AD" pin="AD13" pad="G26"/>
<connect gate="-AD" pin="AD14" pad="G25"/>
<connect gate="-AD" pin="AD15" pad="F26"/>
<connect gate="-AD" pin="AD16" pad="F25"/>
<connect gate="-AD" pin="AD17" pad="F24"/>
<connect gate="-AD" pin="AD18" pad="E24"/>
<connect gate="-AD" pin="AD19" pad="E23"/>
<connect gate="-AD" pin="AD2" pad="K24"/>
<connect gate="-AD" pin="AD20" pad="D24"/>
<connect gate="-AD" pin="AD21" pad="C25"/>
<connect gate="-AD" pin="AD22" pad="C24"/>
<connect gate="-AD" pin="AD23" pad="B24"/>
<connect gate="-AD" pin="AD24" pad="E26"/>
<connect gate="-AD" pin="AD25" pad="E25"/>
<connect gate="-AD" pin="AD26" pad="D26"/>
<connect gate="-AD" pin="AD27" pad="D25"/>
<connect gate="-AD" pin="AD28" pad="C26"/>
<connect gate="-AD" pin="AD29" pad="B26"/>
<connect gate="-AD" pin="AD3" pad="K25"/>
<connect gate="-AD" pin="AD30" pad="B25"/>
<connect gate="-AD" pin="AD31" pad="A25"/>
<connect gate="-AD" pin="AD4" pad="J24"/>
<connect gate="-AD" pin="AD5" pad="H24"/>
<connect gate="-AD" pin="AD6" pad="G24"/>
<connect gate="-AD" pin="AD7" pad="G23"/>
<connect gate="-AD" pin="AD8" pad="K26"/>
<connect gate="-AD" pin="AD9" pad="J26"/>
<connect gate="-C" pin="!ADV" pad="B19"/>
<connect gate="-C" pin="!BAA" pad="A22"/>
<connect gate="-C" pin="!BC0" pad="M25"/>
<connect gate="-C" pin="!BC1" pad="M26"/>
<connect gate="-C" pin="!BC2" pad="L26"/>
<connect gate="-C" pin="!BC3" pad="M24"/>
<connect gate="-C" pin="!BREQ" pad="B22"/>
<connect gate="-C" pin="!BRKIN" pad="H3"/>
<connect gate="-C" pin="!BRKOUT" pad="J3"/>
<connect gate="-C" pin="!CAS" pad="N25"/>
<connect gate="-C" pin="!CKE" pad="P26"/>
<connect gate="-C" pin="!CMDELAY" pad="B21"/>
<connect gate="-C" pin="!CS0" pad="AB24"/>
<connect gate="-C" pin="!CS1" pad="AC26"/>
<connect gate="-C" pin="!CS2" pad="AB25"/>
<connect gate="-C" pin="!CS3" pad="AA24"/>
<connect gate="-C" pin="!CS4" pad="Y23"/>
<connect gate="-C" pin="!CS5" pad="R26"/>
<connect gate="-C" pin="!CS6" pad="P24"/>
<connect gate="-C" pin="!CSEMU" pad="AC25"/>
<connect gate="-C" pin="!CSFPI" pad="B20"/>
<connect gate="-C" pin="!CSGLB" pad="A21"/>
<connect gate="-C" pin="!CSOVL" pad="C20"/>
<connect gate="-C" pin="!HDRST" pad="A1"/>
<connect gate="-C" pin="!HLDA" pad="A23"/>
<connect gate="-C" pin="!HOLD" pad="C22"/>
<connect gate="-C" pin="!MR_W" pad="C21"/>
<connect gate="-C" pin="!NMI" pad="B2"/>
<connect gate="-C" pin="!OCDSE" pad="H2"/>
<connect gate="-C" pin="!PORST" pad="C3"/>
<connect gate="-C" pin="!RAS" pad="P25"/>
<connect gate="-C" pin="!RD" pad="AB26"/>
<connect gate="-C" pin="!RDWR" pad="N24"/>
<connect gate="-C" pin="!RMW" pad="AB23"/>
<connect gate="-C" pin="!SVM" pad="D20"/>
<connect gate="-C" pin="!TM_CTRL1" pad="C15"/>
<connect gate="-C" pin="!TM_CTRL2" pad="C12"/>
<connect gate="-C" pin="!WAIT" pad="C19"/>
<connect gate="-C" pin="ACLK" pad="M23"/>
<connect gate="-C" pin="ALE" pad="A20"/>
<connect gate="-C" pin="CFG0" pad="K2"/>
<connect gate="-C" pin="CFG1" pad="K3"/>
<connect gate="-C" pin="CFG2" pad="J1"/>
<connect gate="-C" pin="CFG3" pad="J2"/>
<connect gate="-C" pin="CLK42" pad="D12"/>
<connect gate="-C" pin="CPUCLK" pad="C2"/>
<connect gate="-C" pin="EBUCLK" pad="N26"/>
<connect gate="-C" pin="MII_MDIO" pad="A10"/>
<connect gate="-C" pin="MII_RXCLK" pad="C11"/>
<connect gate="-C" pin="MII_TXCLK" pad="A11"/>
<connect gate="-C" pin="PLL42_CTRL" pad="B12"/>
<connect gate="-C" pin="PLL96_CTRL" pad="B15"/>
<connect gate="-C" pin="RESERVED@1" pad="A26"/>
<connect gate="-C" pin="RESERVED@2" pad="D15"/>
<connect gate="-C" pin="RESERVED@3" pad="AE26"/>
<connect gate="-C" pin="RESERVED@4" pad="AF9"/>
<connect gate="-C" pin="RESERVED@5" pad="AF26"/>
<connect gate="-C" pin="TESTMODE" pad="AE9"/>
<connect gate="-C" pin="VCOMREF" pad="AD10"/>
<connect gate="-C" pin="VDDDRAM@1" pad="A17"/>
<connect gate="-C" pin="VDDDRAM@2" pad="AF13"/>
<connect gate="-C" pin="VDDOSC" pad="B14"/>
<connect gate="-C" pin="VDDPLL42" pad="A12"/>
<connect gate="-C" pin="VDDPLL96" pad="B13"/>
<connect gate="-C" pin="VLMUREF" pad="A16"/>
<connect gate="-C" pin="VSSOSC" pad="C14"/>
<connect gate="-C" pin="VSSPLL42" pad="C13"/>
<connect gate="-C" pin="VSSPLL96" pad="A13"/>
<connect gate="-C" pin="XTAL1" pad="A15"/>
<connect gate="-C" pin="XTAL2" pad="A14"/>
<connect gate="-JTAG" pin="!TRST" pad="AE8"/>
<connect gate="-JTAG" pin="OCDS2BRK0" pad="G2"/>
<connect gate="-JTAG" pin="OCDS2BRK1" pad="G3"/>
<connect gate="-JTAG" pin="OCDS2BRK2" pad="G4"/>
<connect gate="-JTAG" pin="OCDS2PC0" pad="G1"/>
<connect gate="-JTAG" pin="OCDS2PC1" pad="F1"/>
<connect gate="-JTAG" pin="OCDS2PC2" pad="F2"/>
<connect gate="-JTAG" pin="OCDS2PC3" pad="E1"/>
<connect gate="-JTAG" pin="OCDS2PC4" pad="D1"/>
<connect gate="-JTAG" pin="OCDS2PC5" pad="F3"/>
<connect gate="-JTAG" pin="OCDS2PC6" pad="E2"/>
<connect gate="-JTAG" pin="OCDS2PC7" pad="C1"/>
<connect gate="-JTAG" pin="OCDS2PS0" pad="E3"/>
<connect gate="-JTAG" pin="OCDS2PS1" pad="D2"/>
<connect gate="-JTAG" pin="OCDS2PS2" pad="B1"/>
<connect gate="-JTAG" pin="OCDS2PS3" pad="E4"/>
<connect gate="-JTAG" pin="OCDS2PS4" pad="D3"/>
<connect gate="-JTAG" pin="TCK" pad="AF7"/>
<connect gate="-JTAG" pin="TDI" pad="AD9"/>
<connect gate="-JTAG" pin="TDO" pad="AF8"/>
<connect gate="-JTAG" pin="TMS" pad="AD8"/>
<connect gate="-P0" pin="0" pad="K1"/>
<connect gate="-P0" pin="1" pad="L3"/>
<connect gate="-P0" pin="10" pad="N3"/>
<connect gate="-P0" pin="11" pad="P1"/>
<connect gate="-P0" pin="12" pad="P2"/>
<connect gate="-P0" pin="13" pad="P3"/>
<connect gate="-P0" pin="14" pad="R1"/>
<connect gate="-P0" pin="15" pad="R2"/>
<connect gate="-P0" pin="2" pad="L2"/>
<connect gate="-P0" pin="3" pad="L1"/>
<connect gate="-P0" pin="4" pad="M1"/>
<connect gate="-P0" pin="5" pad="M2"/>
<connect gate="-P0" pin="6" pad="M3"/>
<connect gate="-P0" pin="7" pad="M4"/>
<connect gate="-P0" pin="8" pad="N1"/>
<connect gate="-P0" pin="9" pad="N2"/>
<connect gate="-P1" pin="0" pad="A7"/>
<connect gate="-P1" pin="1" pad="B7"/>
<connect gate="-P1" pin="10" pad="D5"/>
<connect gate="-P1" pin="11" pad="A4"/>
<connect gate="-P1" pin="12" pad="C4"/>
<connect gate="-P1" pin="13" pad="A3"/>
<connect gate="-P1" pin="14" pad="B3"/>
<connect gate="-P1" pin="15" pad="A2"/>
<connect gate="-P1" pin="2" pad="C7"/>
<connect gate="-P1" pin="3" pad="D7"/>
<connect gate="-P1" pin="4" pad="A6"/>
<connect gate="-P1" pin="5" pad="B6"/>
<connect gate="-P1" pin="6" pad="C6"/>
<connect gate="-P1" pin="7" pad="A5"/>
<connect gate="-P1" pin="8" pad="B5"/>
<connect gate="-P1" pin="9" pad="C5"/>
<connect gate="-P2" pin="0" pad="C18"/>
<connect gate="-P2" pin="1" pad="A19"/>
<connect gate="-P2" pin="10" pad="A9"/>
<connect gate="-P2" pin="11" pad="B9"/>
<connect gate="-P2" pin="12" pad="A8"/>
<connect gate="-P2" pin="13" pad="C9"/>
<connect gate="-P2" pin="14" pad="B8"/>
<connect gate="-P2" pin="15" pad="C8"/>
<connect gate="-P2" pin="2" pad="B18"/>
<connect gate="-P2" pin="3" pad="A18"/>
<connect gate="-P2" pin="4" pad="C17"/>
<connect gate="-P2" pin="5" pad="B17"/>
<connect gate="-P2" pin="6" pad="C16"/>
<connect gate="-P2" pin="7" pad="B16"/>
<connect gate="-P2" pin="8" pad="B10"/>
<connect gate="-P2" pin="9" pad="C10"/>
<connect gate="-P3" pin="0" pad="R3"/>
<connect gate="-P3" pin="1" pad="R4"/>
<connect gate="-P3" pin="10" pad="W2"/>
<connect gate="-P3" pin="11" pad="W3"/>
<connect gate="-P3" pin="12" pad="Y1"/>
<connect gate="-P3" pin="13" pad="Y2"/>
<connect gate="-P3" pin="14" pad="Y3"/>
<connect gate="-P3" pin="15" pad="X4"/>
<connect gate="-P3" pin="2" pad="T1"/>
<connect gate="-P3" pin="3" pad="T3"/>
<connect gate="-P3" pin="4" pad="U1"/>
<connect gate="-P3" pin="5" pad="U2"/>
<connect gate="-P3" pin="6" pad="U3"/>
<connect gate="-P3" pin="7" pad="V1"/>
<connect gate="-P3" pin="8" pad="V2"/>
<connect gate="-P3" pin="9" pad="V3"/>
<connect gate="-P4" pin="0" pad="AA1"/>
<connect gate="-P4" pin="1" pad="AA2"/>
<connect gate="-P4" pin="10" pad="AD1"/>
<connect gate="-P4" pin="11" pad="AD2"/>
<connect gate="-P4" pin="12" pad="AE1"/>
<connect gate="-P4" pin="13" pad="AE2"/>
<connect gate="-P4" pin="14" pad="AD3"/>
<connect gate="-P4" pin="15" pad="AF2"/>
<connect gate="-P4" pin="2" pad="AA3"/>
<connect gate="-P4" pin="3" pad="AB1"/>
<connect gate="-P4" pin="4" pad="AB2"/>
<connect gate="-P4" pin="5" pad="AB3"/>
<connect gate="-P4" pin="6" pad="AB4"/>
<connect gate="-P4" pin="7" pad="AC1"/>
<connect gate="-P4" pin="8" pad="AC2"/>
<connect gate="-P4" pin="9" pad="AC3"/>
<connect gate="-P5" pin="0" pad="AF1"/>
<connect gate="-P5" pin="1" pad="AE3"/>
<connect gate="-P5" pin="10" pad="AC7"/>
<connect gate="-P5" pin="11" pad="AF5"/>
<connect gate="-P5" pin="12" pad="AE6"/>
<connect gate="-P5" pin="13" pad="AD7"/>
<connect gate="-P5" pin="14" pad="AF6"/>
<connect gate="-P5" pin="15" pad="AE7"/>
<connect gate="-P5" pin="2" pad="AD4"/>
<connect gate="-P5" pin="3" pad="AC5"/>
<connect gate="-P5" pin="4" pad="AF3"/>
<connect gate="-P5" pin="5" pad="AE4"/>
<connect gate="-P5" pin="6" pad="AD5"/>
<connect gate="-P5" pin="7" pad="AF4"/>
<connect gate="-P5" pin="8" pad="AE5"/>
<connect gate="-P5" pin="9" pad="AD6"/>
<connect gate="-PCI" pin="!P_CBE0" pad="AC24"/>
<connect gate="-PCI" pin="!P_CBE1" pad="AF21"/>
<connect gate="-PCI" pin="!P_CBE2" pad="AF18"/>
<connect gate="-PCI" pin="!P_CBE3" pad="AF15"/>
<connect gate="-PCI" pin="!P_DEVSEL" pad="AF19"/>
<connect gate="-PCI" pin="!P_FRAME" pad="AD18"/>
<connect gate="-PCI" pin="!P_GNT" pad="AD11"/>
<connect gate="-PCI" pin="!P_INTA" pad="AE10"/>
<connect gate="-PCI" pin="!P_INTB" pad="AF10"/>
<connect gate="-PCI" pin="!P_IRDY" pad="AE18"/>
<connect gate="-PCI" pin="!P_LOCK" pad="AE19"/>
<connect gate="-PCI" pin="!P_PERR" pad="AF20"/>
<connect gate="-PCI" pin="!P_PME" pad="AC12"/>
<connect gate="-PCI" pin="!P_REQ" pad="AE11"/>
<connect gate="-PCI" pin="!P_SERR" pad="AE20"/>
<connect gate="-PCI" pin="!P_STOP" pad="AC20"/>
<connect gate="-PCI" pin="!P_TRDY" pad="AD19"/>
<connect gate="-PCI" pin="P_CLK33" pad="AF11"/>
<connect gate="-PCI" pin="P_IDSEL" pad="AC15"/>
<connect gate="-PCI" pin="P_PAR" pad="AD20"/>
<connect gate="-P_AD" pin="AD0" pad="AD26"/>
<connect gate="-P_AD" pin="AD1" pad="AE25"/>
<connect gate="-P_AD" pin="AD10" pad="AE22"/>
<connect gate="-P_AD" pin="AD11" pad="AD22"/>
<connect gate="-P_AD" pin="AD12" pad="AF22"/>
<connect gate="-P_AD" pin="AD13" pad="AC22"/>
<connect gate="-P_AD" pin="AD14" pad="AE21"/>
<connect gate="-P_AD" pin="AD15" pad="AD21"/>
<connect gate="-P_AD" pin="AD16" pad="AE17"/>
<connect gate="-P_AD" pin="AD17" pad="AF17"/>
<connect gate="-P_AD" pin="AD18" pad="AD17"/>
<connect gate="-P_AD" pin="AD19" pad="AE16"/>
<connect gate="-P_AD" pin="AD2" pad="AD25"/>
<connect gate="-P_AD" pin="AD20" pad="AD16"/>
<connect gate="-P_AD" pin="AD21" pad="AF16"/>
<connect gate="-P_AD" pin="AD22" pad="AD15"/>
<connect gate="-P_AD" pin="AD23" pad="AE15"/>
<connect gate="-P_AD" pin="AD24" pad="AE14"/>
<connect gate="-P_AD" pin="AD25" pad="AF14"/>
<connect gate="-P_AD" pin="AD26" pad="AD14"/>
<connect gate="-P_AD" pin="AD27" pad="AE13"/>
<connect gate="-P_AD" pin="AD28" pad="AD13"/>
<connect gate="-P_AD" pin="AD29" pad="AE12"/>
<connect gate="-P_AD" pin="AD3" pad="AF25"/>
<connect gate="-P_AD" pin="AD30" pad="AD12"/>
<connect gate="-P_AD" pin="AD31" pad="AF12"/>
<connect gate="-P_AD" pin="AD4" pad="AE24"/>
<connect gate="-P_AD" pin="AD5" pad="AF24"/>
<connect gate="-P_AD" pin="AD6" pad="AD24"/>
<connect gate="-P_AD" pin="AD7" pad="AE23"/>
<connect gate="-P_AD" pin="AD8" pad="AF23"/>
<connect gate="-P_AD" pin="AD9" pad="AD23"/>
<connect gate="-VSS1" pin="VSS" pad="D4"/>
<connect gate="-VSS10" pin="VSS" pad="V4"/>
<connect gate="-VSS11" pin="VSS" pad="V23"/>
<connect gate="-VSS12" pin="VSS" pad="AC4"/>
<connect gate="-VSS13" pin="VSS" pad="AC9"/>
<connect gate="-VSS14" pin="VSS" pad="AC14"/>
<connect gate="-VSS15" pin="VSS" pad="AC18"/>
<connect gate="-VSS16" pin="VSS" pad="AC23"/>
<connect gate="-VSS17" pin="VSS" pad="L11"/>
<connect gate="-VSS18" pin="VSS" pad="L12"/>
<connect gate="-VSS19" pin="VSS" pad="L13"/>
<connect gate="-VSS2" pin="VSS" pad="D9"/>
<connect gate="-VSS20" pin="VSS" pad="L14"/>
<connect gate="-VSS21" pin="VSS" pad="L15"/>
<connect gate="-VSS22" pin="VSS" pad="L16"/>
<connect gate="-VSS23" pin="VSS" pad="M11"/>
<connect gate="-VSS24" pin="VSS" pad="M12"/>
<connect gate="-VSS25" pin="VSS" pad="M13"/>
<connect gate="-VSS26" pin="VSS" pad="M14"/>
<connect gate="-VSS27" pin="VSS" pad="M15"/>
<connect gate="-VSS28" pin="VSS" pad="M16"/>
<connect gate="-VSS29" pin="VSS" pad="N11"/>
<connect gate="-VSS3" pin="VSS" pad="D13"/>
<connect gate="-VSS30" pin="VSS" pad="N12"/>
<connect gate="-VSS31" pin="VSS" pad="N13"/>
<connect gate="-VSS32" pin="VSS" pad="N14"/>
<connect gate="-VSS33" pin="VSS" pad="N15"/>
<connect gate="-VSS34" pin="VSS" pad="N16"/>
<connect gate="-VSS35" pin="VSS" pad="P11"/>
<connect gate="-VSS36" pin="VSS" pad="P12"/>
<connect gate="-VSS37" pin="VSS" pad="P13"/>
<connect gate="-VSS38" pin="VSS" pad="P14"/>
<connect gate="-VSS39" pin="VSS" pad="P15"/>
<connect gate="-VSS4" pin="VSS" pad="D18"/>
<connect gate="-VSS40" pin="VSS" pad="P16"/>
<connect gate="-VSS41" pin="VSS" pad="R11"/>
<connect gate="-VSS42" pin="VSS" pad="R12"/>
<connect gate="-VSS43" pin="VSS" pad="R13"/>
<connect gate="-VSS44" pin="VSS" pad="R14"/>
<connect gate="-VSS45" pin="VSS" pad="R15"/>
<connect gate="-VSS46" pin="VSS" pad="R16"/>
<connect gate="-VSS47" pin="VSS" pad="T11"/>
<connect gate="-VSS48" pin="VSS" pad="T12"/>
<connect gate="-VSS49" pin="VSS" pad="T13"/>
<connect gate="-VSS5" pin="VSS" pad="D23"/>
<connect gate="-VSS50" pin="VSS" pad="T14"/>
<connect gate="-VSS51" pin="VSS" pad="T15"/>
<connect gate="-VSS52" pin="VSS" pad="T16"/>
<connect gate="-VSS6" pin="VSS" pad="J4"/>
<connect gate="-VSS7" pin="VSS" pad="J23"/>
<connect gate="-VSS8" pin="VSS" pad="N23"/>
<connect gate="-VSS9" pin="VSS" pad="P4"/>
<connect gate="VDD1" pin="VDD" pad="H1"/>
<connect gate="VDD10" pin="VDD" pad="D21"/>
<connect gate="VDD11" pin="VDD" pad="F23"/>
<connect gate="VDD12" pin="VDD" pad="K4"/>
<connect gate="VDD13" pin="VDD" pad="K23"/>
<connect gate="VDD14" pin="VDD" pad="U4"/>
<connect gate="VDD15" pin="VDD" pad="U23"/>
<connect gate="VDD16" pin="VDD" pad="AA4"/>
<connect gate="VDD17" pin="VDD" pad="AA23"/>
<connect gate="VDD18" pin="VDD" pad="AC6"/>
<connect gate="VDD19" pin="VDD" pad="AC10"/>
<connect gate="VDD2" pin="VDD" pad="W1"/>
<connect gate="VDD20" pin="VDD" pad="AC17"/>
<connect gate="VDD21" pin="VDD" pad="AC21"/>
<connect gate="VDD3" pin="VDD" pad="T2"/>
<connect gate="VDD4" pin="VDD" pad="B4"/>
<connect gate="VDD5" pin="VDD" pad="B11"/>
<connect gate="VDD6" pin="VDD" pad="D6"/>
<connect gate="VDD7" pin="VDD" pad="F4"/>
<connect gate="VDD8" pin="VDD" pad="D10"/>
<connect gate="VDD9" pin="VDD" pad="D17"/>
<connect gate="VDDP1" pin="VDDP" pad="D8"/>
<connect gate="VDDP10" pin="VDDP" pad="N4"/>
<connect gate="VDDP11" pin="VDDP" pad="P23"/>
<connect gate="VDDP12" pin="VDDP" pad="T4"/>
<connect gate="VDDP13" pin="VDDP" pad="T23"/>
<connect gate="VDDP14" pin="VDDP" pad="W4"/>
<connect gate="VDDP15" pin="VDDP" pad="W23"/>
<connect gate="VDDP16" pin="VDDP" pad="AC8"/>
<connect gate="VDDP17" pin="VDDP" pad="AC11"/>
<connect gate="VDDP18" pin="VDDP" pad="AC13"/>
<connect gate="VDDP19" pin="VDDP" pad="AC16"/>
<connect gate="VDDP2" pin="VDDP" pad="D11"/>
<connect gate="VDDP20" pin="VDDP" pad="AC19"/>
<connect gate="VDDP3" pin="VDDP" pad="D14"/>
<connect gate="VDDP4" pin="VDDP" pad="D16"/>
<connect gate="VDDP5" pin="VDDP" pad="D19"/>
<connect gate="VDDP6" pin="VDDP" pad="H4"/>
<connect gate="VDDP7" pin="VDDP" pad="H23"/>
<connect gate="VDDP8" pin="VDDP" pad="L4"/>
<connect gate="VDDP9" pin="VDDP" pad="L23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC191*" prefix="IC">
<description>&lt;b&gt;32 bit TriCore based microcontroller/DSP&lt;/b&gt;&lt;p&gt;
 which is mainly designed for automotive telematics applications.&lt;br&gt;
Source: http://www.infineon.com .. TC1910_DS_V1.0.pdf / TC1912_DS_V1.0.pdf</description>
<gates>
<gate name="-C" symbol="TC1910-1"/>
<gate name="-JTAG" symbol="JTAG-OCSD-1"/>
<gate name="-P0" symbol="PORT0-10_12"/>
<gate name="-P1" symbol="PORT1-10_12"/>
<gate name="-P2" symbol="PORT2-10_12"/>
<gate name="-P3" symbol="PORT3-10_12"/>
<gate name="HS1" symbol="HEATSINK"/>
<gate name="HS2" symbol="HEATSINK"/>
<gate name="HS3" symbol="HEATSINK"/>
<gate name="HS4" symbol="HEATSINK"/>
<gate name="HS5" symbol="HEATSINK"/>
<gate name="HS6" symbol="HEATSINK"/>
<gate name="HS7" symbol="HEATSINK"/>
<gate name="HS8" symbol="HEATSINK"/>
<gate name="HS9" symbol="HEATSINK"/>
<gate name="HS10" symbol="HEATSINK"/>
<gate name="HS11" symbol="HEATSINK"/>
<gate name="HS12" symbol="HEATSINK"/>
<gate name="HS13" symbol="HEATSINK"/>
<gate name="HS14" symbol="HEATSINK"/>
<gate name="HS15" symbol="HEATSINK"/>
<gate name="HS0" symbol="HEATSINK"/>
<gate name="-A" symbol="A23"/>
<gate name="-AD" symbol="AD31"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="-A" pin="A0" pad="R3"/>
<connect gate="-A" pin="A1" pad="P4"/>
<connect gate="-A" pin="A10" pad="N1"/>
<connect gate="-A" pin="A11" pad="M4"/>
<connect gate="-A" pin="A12" pad="M3"/>
<connect gate="-A" pin="A13" pad="L4"/>
<connect gate="-A" pin="A14" pad="M2"/>
<connect gate="-A" pin="A15" pad="M1"/>
<connect gate="-A" pin="A16" pad="L3"/>
<connect gate="-A" pin="A17" pad="L1"/>
<connect gate="-A" pin="A18" pad="L2"/>
<connect gate="-A" pin="A19" pad="K4"/>
<connect gate="-A" pin="A2" pad="T1"/>
<connect gate="-A" pin="A20" pad="K3"/>
<connect gate="-A" pin="A21" pad="J4"/>
<connect gate="-A" pin="A22" pad="K2"/>
<connect gate="-A" pin="A23" pad="J3"/>
<connect gate="-A" pin="A3" pad="R2"/>
<connect gate="-A" pin="A4" pad="R1"/>
<connect gate="-A" pin="A5" pad="P3"/>
<connect gate="-A" pin="A6" pad="P2"/>
<connect gate="-A" pin="A7" pad="P1"/>
<connect gate="-A" pin="A8" pad="N3"/>
<connect gate="-A" pin="A9" pad="N2"/>
<connect gate="-AD" pin="AD0" pad="H4"/>
<connect gate="-AD" pin="AD1" pad="J2"/>
<connect gate="-AD" pin="AD10" pad="G3"/>
<connect gate="-AD" pin="AD11" pad="G2"/>
<connect gate="-AD" pin="AD12" pad="F4"/>
<connect gate="-AD" pin="AD13" pad="C1"/>
<connect gate="-AD" pin="AD14" pad="F3"/>
<connect gate="-AD" pin="AD15" pad="F2"/>
<connect gate="-AD" pin="AD16" pad="E3"/>
<connect gate="-AD" pin="AD17" pad="B1"/>
<connect gate="-AD" pin="AD18" pad="E2"/>
<connect gate="-AD" pin="AD19" pad="E4"/>
<connect gate="-AD" pin="AD2" pad="H1"/>
<connect gate="-AD" pin="AD20" pad="A1"/>
<connect gate="-AD" pin="AD21" pad="D2"/>
<connect gate="-AD" pin="AD22" pad="D3"/>
<connect gate="-AD" pin="AD23" pad="C2"/>
<connect gate="-AD" pin="AD24" pad="C3"/>
<connect gate="-AD" pin="AD25" pad="B2"/>
<connect gate="-AD" pin="AD26" pad="A2"/>
<connect gate="-AD" pin="AD27" pad="B3"/>
<connect gate="-AD" pin="AD28" pad="A3"/>
<connect gate="-AD" pin="AD29" pad="A4"/>
<connect gate="-AD" pin="AD3" pad="H3"/>
<connect gate="-AD" pin="AD30" pad="B4"/>
<connect gate="-AD" pin="AD31" pad="C4"/>
<connect gate="-AD" pin="AD4" pad="H2"/>
<connect gate="-AD" pin="AD5" pad="G1"/>
<connect gate="-AD" pin="AD6" pad="G4"/>
<connect gate="-AD" pin="AD7" pad="F1"/>
<connect gate="-AD" pin="AD8" pad="E1"/>
<connect gate="-AD" pin="AD9" pad="D1"/>
<connect gate="-C" pin="!ADV" pad="N9"/>
<connect gate="-C" pin="!BAA" pad="P8"/>
<connect gate="-C" pin="!BC0" pad="N6"/>
<connect gate="-C" pin="!BC1" pad="R5"/>
<connect gate="-C" pin="!BC2" pad="T4"/>
<connect gate="-C" pin="!BC3" pad="T3"/>
<connect gate="-C" pin="!CAS" pad="T2"/>
<connect gate="-C" pin="!CMDELAY" pad="T9"/>
<connect gate="-C" pin="!CS0" pad="R7"/>
<connect gate="-C" pin="!CS1" pad="N7"/>
<connect gate="-C" pin="!CS2" pad="P7"/>
<connect gate="-C" pin="!CS3" pad="T6"/>
<connect gate="-C" pin="!CS4" pad="R6"/>
<connect gate="-C" pin="!CS5" pad="T5"/>
<connect gate="-C" pin="!CS6" pad="P6"/>
<connect gate="-C" pin="!CSEMU" pad="R8"/>
<connect gate="-C" pin="!CSGLB" pad="N8"/>
<connect gate="-C" pin="!CSOVL" pad="T8"/>
<connect gate="-C" pin="!HRST" pad="B13"/>
<connect gate="-C" pin="!MR_W" pad="R9"/>
<connect gate="-C" pin="!NMI" pad="A13"/>
<connect gate="-C" pin="!PORST" pad="C13"/>
<connect gate="-C" pin="!RAS" pad="N5"/>
<connect gate="-C" pin="!RD" pad="R4"/>
<connect gate="-C" pin="!RD_WR" pad="P5"/>
<connect gate="-C" pin="!SCANMODE" pad="J14"/>
<connect gate="-C" pin="!WAIT" pad="T7"/>
<connect gate="-C" pin="AI0+" pad="D9"/>
<connect gate="-C" pin="AI0-" pad="B9"/>
<connect gate="-C" pin="AI1+" pad="C10"/>
<connect gate="-C" pin="AI1-" pad="B10"/>
<connect gate="-C" pin="ALE" pad="R10"/>
<connect gate="-C" pin="AO0+" pad="C11"/>
<connect gate="-C" pin="AO0-" pad="B12"/>
<connect gate="-C" pin="AO1+" pad="B11"/>
<connect gate="-C" pin="AO1-" pad="D11"/>
<connect gate="-C" pin="BFCLK0" pad="K1"/>
<connect gate="-C" pin="BYPASS" pad="A12"/>
<connect gate="-C" pin="CEXT" pad="D12"/>
<connect gate="-C" pin="CKE" pad="P9"/>
<connect gate="-C" pin="CLKOUT" pad="A14"/>
<connect gate="-C" pin="CODEC_DIS" pad="C12"/>
<connect gate="-C" pin="EBUCLK" pad="J1"/>
<connect gate="-C" pin="PLLCTRL_AO" pad="D8"/>
<connect gate="-C" pin="TM_CTRL0" pad="C7"/>
<connect gate="-C" pin="TM_CTRL1" pad="C5"/>
<connect gate="-C" pin="VAGND_GOD" pad="C9"/>
<connect gate="-C" pin="VAREF_GOD" pad="D10"/>
<connect gate="-C" pin="VDDPLL" pad="B6"/>
<connect gate="-C" pin="VDDR" pad="D6"/>
<connect gate="-C" pin="VDDSB" pad="L13"/>
<connect gate="-C" pin="VDD_COD0/1" pad="A10"/>
<connect gate="-C" pin="VDD_GUARD" pad="B8"/>
<connect gate="-C" pin="VDD_OSCI" pad="D7"/>
<connect gate="-C" pin="VDD_PLL" pad="A9"/>
<connect gate="-C" pin="VDD_PWR2@1" pad="G7"/>
<connect gate="-C" pin="VDD_PWR2@2" pad="G10"/>
<connect gate="-C" pin="VDD_PWR2@3" pad="K7"/>
<connect gate="-C" pin="VDD_PWR2@4" pad="K10"/>
<connect gate="-C" pin="VDD_PWR@1" pad="D4"/>
<connect gate="-C" pin="VDD_PWR@2" pad="D13"/>
<connect gate="-C" pin="VDD_PWR@3" pad="H7"/>
<connect gate="-C" pin="VDD_PWR@4" pad="N4"/>
<connect gate="-C" pin="VDD_PWR@5" pad="N13"/>
<connect gate="-C" pin="VDD_RTC" pad="A5"/>
<connect gate="-C" pin="VSSA_COD0/1" pad="A11"/>
<connect gate="-C" pin="VSSPLL" pad="A8"/>
<connect gate="-C" pin="VSS_32K" pad="B5"/>
<connect gate="-C" pin="VSS_GND@1" pad="G8"/>
<connect gate="-C" pin="VSS_GND@2" pad="G9"/>
<connect gate="-C" pin="VSS_GND@3" pad="H8"/>
<connect gate="-C" pin="VSS_GND@4" pad="H9"/>
<connect gate="-C" pin="VSS_GND@5" pad="J8"/>
<connect gate="-C" pin="VSS_GND@6" pad="J9"/>
<connect gate="-C" pin="VSS_GUARD" pad="C8"/>
<connect gate="-C" pin="VSS_PLL" pad="B7"/>
<connect gate="-C" pin="XTAL1" pad="A6"/>
<connect gate="-C" pin="XTAL2" pad="A7"/>
<connect gate="-C" pin="XTAL3" pad="D5"/>
<connect gate="-C" pin="XTAL4" pad="C6"/>
<connect gate="-JTAG" pin="!BRKIN" pad="R13"/>
<connect gate="-JTAG" pin="!BRKOUT" pad="P12"/>
<connect gate="-JTAG" pin="!OCDSE" pad="T14"/>
<connect gate="-JTAG" pin="!TRST" pad="T16"/>
<connect gate="-JTAG" pin="TCK" pad="R15"/>
<connect gate="-JTAG" pin="TDI" pad="T15"/>
<connect gate="-JTAG" pin="TDO" pad="R14"/>
<connect gate="-JTAG" pin="TMS" pad="P13"/>
<connect gate="-P0" pin="0/EXI0IN" pad="M14"/>
<connect gate="-P0" pin="1/EXI1IN/DATA_IN" pad="M15"/>
<connect gate="-P0" pin="2/EXI2IN/DATA_OUT" pad="M16"/>
<connect gate="-P0" pin="3/EXI3IN/MCLK" pad="L14"/>
<connect gate="-P0" pin="4/GPIO/SCLK" pad="L15"/>
<connect gate="-P0" pin="5/GPIO/LRCK" pad="K13"/>
<connect gate="-P0" pin="6/GPIO/MUTE0" pad="L16"/>
<connect gate="-P0" pin="7/GPIO/MUTE1" pad="K14"/>
<connect gate="-P1" pin="0/GPIO" pad="P14"/>
<connect gate="-P1" pin="1/GPIO" pad="R16"/>
<connect gate="-P1" pin="2/GPIO" pad="P15"/>
<connect gate="-P1" pin="3/GPIO" pad="P16"/>
<connect gate="-P1" pin="4/GPIO" pad="N14"/>
<connect gate="-P1" pin="5/GPIO" pad="N15"/>
<connect gate="-P1" pin="6/GPIO" pad="N16"/>
<connect gate="-P1" pin="7/GPIO" pad="M13"/>
<connect gate="-P2" pin="0/GPIO/RXDCAN0" pad="A16"/>
<connect gate="-P2" pin="1/GPIO/TXDCAN0" pad="G13"/>
<connect gate="-P2" pin="10/RXD0" pad="D15"/>
<connect gate="-P2" pin="11/TXD0" pad="E14"/>
<connect gate="-P2" pin="12/SCLK" pad="D14"/>
<connect gate="-P2" pin="13/MRST" pad="E13"/>
<connect gate="-P2" pin="14/MTSR" pad="C14"/>
<connect gate="-P2" pin="15/GPIO/EXI4IN/PLL_CLC.LOCK" pad="B14"/>
<connect gate="-P2" pin="2/GPIO/RXDCAN1" pad="G14"/>
<connect gate="-P2" pin="3/GPIO/TXDCAN1" pad="A15"/>
<connect gate="-P2" pin="4/GPIO" pad="F15"/>
<connect gate="-P2" pin="5/GPIO" pad="B15"/>
<connect gate="-P2" pin="6/SCL" pad="E15"/>
<connect gate="-P2" pin="7/SDA" pad="C15"/>
<connect gate="-P2" pin="8/GPIO" pad="F13"/>
<connect gate="-P2" pin="9/GPIO" pad="F14"/>
<connect gate="-P3" pin="0/GPTU.0" pad="J13"/>
<connect gate="-P3" pin="1/GPTU.1" pad="K16"/>
<connect gate="-P3" pin="10/GPIO/RXD2" pad="G16"/>
<connect gate="-P3" pin="11/GPIO/OSCBYP/TXD2" pad="E16"/>
<connect gate="-P3" pin="12/EXI5IN/HWCFG0" pad="F16"/>
<connect gate="-P3" pin="13/EXI6IN/HWCFG1" pad="G15"/>
<connect gate="-P3" pin="14/EXI7IN/HWCFG2" pad="C16"/>
<connect gate="-P3" pin="15/GPIO" pad="B16"/>
<connect gate="-P3" pin="2/GPTU.2" pad="K15"/>
<connect gate="-P3" pin="3/GPTU.3" pad="J16"/>
<connect gate="-P3" pin="4/GPTU.4" pad="H13"/>
<connect gate="-P3" pin="5/GPTU.5" pad="H14"/>
<connect gate="-P3" pin="6/GPTU.6" pad="J15"/>
<connect gate="-P3" pin="7/GPTU.7" pad="H15"/>
<connect gate="-P3" pin="8/RXD1" pad="H16"/>
<connect gate="-P3" pin="9/TXD1" pad="D16"/>
<connect gate="HS0" pin="HS" pad="N12"/>
<connect gate="HS1" pin="HS" pad="T13"/>
<connect gate="HS10" pin="HS" pad="P10"/>
<connect gate="HS11" pin="HS" pad="N10"/>
<connect gate="HS12" pin="HS" pad="T10"/>
<connect gate="HS13" pin="HS" pad="K9"/>
<connect gate="HS14" pin="HS" pad="K8"/>
<connect gate="HS15" pin="HS" pad="J7"/>
<connect gate="HS2" pin="HS" pad="R12"/>
<connect gate="HS3" pin="HS" pad="T12"/>
<connect gate="HS4" pin="HS" pad="J10"/>
<connect gate="HS5" pin="HS" pad="H10"/>
<connect gate="HS6" pin="HS" pad="P11"/>
<connect gate="HS7" pin="HS" pad="N11"/>
<connect gate="HS8" pin="HS" pad="R11"/>
<connect gate="HS9" pin="HS" pad="T11"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1100" prefix="IC">
<description>&lt;b&gt;32-bit Consumer Class TriCore&lt;/b&gt; Single-Chip Microcontroller&lt;p&gt;
Source: http://www.infineon.com/cmc_upload/documents/010/9915/TC1100_umsu_v10.pdf</description>
<gates>
<gate name="-C" symbol="TC1100"/>
<gate name="-P0" symbol="PORT16"/>
<gate name="-P1" symbol="PORT16"/>
<gate name="-P2" symbol="PORT16"/>
<gate name="-P3" symbol="PORT16"/>
<gate name="-P4" symbol="PORT8"/>
<gate name="-AD" symbol="AD31"/>
<gate name="-A" symbol="A23"/>
<gate name="-JTAG" symbol="JTAG"/>
<gate name="-VSS1" symbol="VSS"/>
<gate name="-VSS2" symbol="VSS"/>
<gate name="-VSS3" symbol="VSS"/>
<gate name="-VSS4" symbol="VSS"/>
<gate name="-VSS5" symbol="VSS"/>
<gate name="-VSS6" symbol="VSS"/>
<gate name="-VSS7" symbol="VSS"/>
<gate name="-VSS8" symbol="VSS"/>
<gate name="-VSS9" symbol="VSS"/>
<gate name="-VSS10" symbol="VSS"/>
<gate name="-VSS11" symbol="VSS"/>
<gate name="-VSS12" symbol="VSS"/>
<gate name="-VSS13" symbol="VSS"/>
<gate name="-VSS14" symbol="VSS"/>
<gate name="-VSS15" symbol="VSS"/>
<gate name="-VSS16" symbol="VSS"/>
<gate name="-VDD1" symbol="VDD"/>
<gate name="-VDD2" symbol="VDD"/>
<gate name="-VDD3" symbol="VDD"/>
<gate name="-VDD4" symbol="VDD"/>
<gate name="-VDD5" symbol="VDD"/>
<gate name="-VDD6" symbol="VDD"/>
<gate name="-VDD7" symbol="VDD"/>
<gate name="-VDD8" symbol="VDD"/>
<gate name="-VDD9" symbol="VDD"/>
<gate name="-VDDP1" symbol="VDDP"/>
<gate name="-VDDP2" symbol="VDDP"/>
<gate name="-VDDP3" symbol="VDDP"/>
<gate name="-VDDP4" symbol="VDDP"/>
<gate name="-VDDP5" symbol="VDDP"/>
<gate name="-VDDP6" symbol="VDDP"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="-A" pin="A0" pad="K1"/>
<connect gate="-A" pin="A1" pad="L1"/>
<connect gate="-A" pin="A10" pad="J3"/>
<connect gate="-A" pin="A11" pad="K3"/>
<connect gate="-A" pin="A12" pad="L3"/>
<connect gate="-A" pin="A13" pad="M3"/>
<connect gate="-A" pin="A14" pad="K4"/>
<connect gate="-A" pin="A15" pad="A8"/>
<connect gate="-A" pin="A16" pad="A9"/>
<connect gate="-A" pin="A17" pad="A10"/>
<connect gate="-A" pin="A18" pad="B10"/>
<connect gate="-A" pin="A19" pad="C10"/>
<connect gate="-A" pin="A2" pad="M1"/>
<connect gate="-A" pin="A20" pad="D10"/>
<connect gate="-A" pin="A21" pad="T4"/>
<connect gate="-A" pin="A22" pad="R4"/>
<connect gate="-A" pin="A23" pad="P4"/>
<connect gate="-A" pin="A3" pad="N1"/>
<connect gate="-A" pin="A4" pad="P1"/>
<connect gate="-A" pin="A5" pad="J2"/>
<connect gate="-A" pin="A6" pad="K2"/>
<connect gate="-A" pin="A7" pad="L2"/>
<connect gate="-A" pin="A8" pad="M2"/>
<connect gate="-A" pin="A9" pad="N2"/>
<connect gate="-AD" pin="AD0" pad="C8"/>
<connect gate="-AD" pin="AD1" pad="C7"/>
<connect gate="-AD" pin="AD10" pad="F1"/>
<connect gate="-AD" pin="AD11" pad="E3"/>
<connect gate="-AD" pin="AD12" pad="F3"/>
<connect gate="-AD" pin="AD13" pad="G1"/>
<connect gate="-AD" pin="AD14" pad="H2"/>
<connect gate="-AD" pin="AD15" pad="G3"/>
<connect gate="-AD" pin="AD16" pad="D7"/>
<connect gate="-AD" pin="AD17" pad="B5"/>
<connect gate="-AD" pin="AD18" pad="A4"/>
<connect gate="-AD" pin="AD19" pad="B4"/>
<connect gate="-AD" pin="AD2" pad="B6"/>
<connect gate="-AD" pin="AD20" pad="C4"/>
<connect gate="-AD" pin="AD21" pad="B3"/>
<connect gate="-AD" pin="AD22" pad="B2"/>
<connect gate="-AD" pin="AD23" pad="B1"/>
<connect gate="-AD" pin="AD24" pad="C1"/>
<connect gate="-AD" pin="AD25" pad="D3"/>
<connect gate="-AD" pin="AD26" pad="E2"/>
<connect gate="-AD" pin="AD27" pad="F2"/>
<connect gate="-AD" pin="AD28" pad="F4"/>
<connect gate="-AD" pin="AD29" pad="G4"/>
<connect gate="-AD" pin="AD3" pad="C6"/>
<connect gate="-AD" pin="AD30" pad="H3"/>
<connect gate="-AD" pin="AD31" pad="G2"/>
<connect gate="-AD" pin="AD4" pad="C5"/>
<connect gate="-AD" pin="AD5" pad="A3"/>
<connect gate="-AD" pin="AD6" pad="A2"/>
<connect gate="-AD" pin="AD7" pad="C3"/>
<connect gate="-AD" pin="AD8" pad="C2"/>
<connect gate="-AD" pin="AD9" pad="D2"/>
<connect gate="-C" pin="!ADV" pad="B11"/>
<connect gate="-C" pin="!BAA" pad="A11"/>
<connect gate="-C" pin="!BC0" pad="A5"/>
<connect gate="-C" pin="!BC1" pad="A6"/>
<connect gate="-C" pin="!BC2" pad="B7"/>
<connect gate="-C" pin="!BC3" pad="A7"/>
<connect gate="-C" pin="!BRKIN" pad="T5"/>
<connect gate="-C" pin="!CAS" pad="D5"/>
<connect gate="-C" pin="!CS0" pad="D9"/>
<connect gate="-C" pin="!CS1" pad="D8"/>
<connect gate="-C" pin="!CS2" pad="C9"/>
<connect gate="-C" pin="!CS3" pad="B8"/>
<connect gate="-C" pin="!CSCOMB" pad="N3"/>
<connect gate="-C" pin="!HDRST" pad="N5"/>
<connect gate="-C" pin="!MR_W" pad="P3"/>
<connect gate="-C" pin="!NMI" pad="T7"/>
<connect gate="-C" pin="!PORST" pad="R5"/>
<connect gate="-C" pin="!RAS" pad="D6"/>
<connect gate="-C" pin="!RD" pad="P2"/>
<connect gate="-C" pin="!RD_WR" pad="T3"/>
<connect gate="-C" pin="!TRCLK" pad="T8"/>
<connect gate="-C" pin="!WAIT" pad="B9"/>
<connect gate="-C" pin="ALE" pad="R3"/>
<connect gate="-C" pin="BFCLKI" pad="D1"/>
<connect gate="-C" pin="BFCLKO" pad="E1"/>
<connect gate="-C" pin="CKE" pad="L4"/>
<connect gate="-C" pin="HWCFG0" pad="M14"/>
<connect gate="-C" pin="HWCFG1" pad="L14"/>
<connect gate="-C" pin="HWCFG2" pad="T6"/>
<connect gate="-C" pin="NC@1" pad="R1"/>
<connect gate="-C" pin="NC@2" pad="T14"/>
<connect gate="-C" pin="NC@3" pad="T15"/>
<connect gate="-C" pin="RESERVED@1" pad="A1"/>
<connect gate="-C" pin="RESERVED@2" pad="A16"/>
<connect gate="-C" pin="RESERVED@3" pad="T1"/>
<connect gate="-C" pin="RESERVED@4" pad="T16"/>
<connect gate="-C" pin="SDCLKI" pad="J1"/>
<connect gate="-C" pin="SDCLKO" pad="H1"/>
<connect gate="-C" pin="VDDOSC" pad="L16"/>
<connect gate="-C" pin="VDDOSC3" pad="P16"/>
<connect gate="-C" pin="VSSOSC" pad="L15"/>
<connect gate="-C" pin="VSSOSC3" pad="R16"/>
<connect gate="-C" pin="XTAL1" pad="M16"/>
<connect gate="-C" pin="XTAL2" pad="N16"/>
<connect gate="-JTAG" pin="!TRST" pad="T11"/>
<connect gate="-JTAG" pin="TCK" pad="T12"/>
<connect gate="-JTAG" pin="TDI" pad="T13"/>
<connect gate="-JTAG" pin="TDO" pad="T10"/>
<connect gate="-JTAG" pin="TMS" pad="T9"/>
<connect gate="-P0" pin="0" pad="N11"/>
<connect gate="-P0" pin="1" pad="P15"/>
<connect gate="-P0" pin="10" pad="R14"/>
<connect gate="-P0" pin="11" pad="N9"/>
<connect gate="-P0" pin="12" pad="P9"/>
<connect gate="-P0" pin="13" pad="P8"/>
<connect gate="-P0" pin="14" pad="N8"/>
<connect gate="-P0" pin="15" pad="P7"/>
<connect gate="-P0" pin="2" pad="P10"/>
<connect gate="-P0" pin="3" pad="M15"/>
<connect gate="-P0" pin="4" pad="R11"/>
<connect gate="-P0" pin="5" pad="R12"/>
<connect gate="-P0" pin="6" pad="R10"/>
<connect gate="-P0" pin="7" pad="N10"/>
<connect gate="-P0" pin="8" pad="R13"/>
<connect gate="-P0" pin="9" pad="R15"/>
<connect gate="-P1" pin="0" pad="D11"/>
<connect gate="-P1" pin="1" pad="C12"/>
<connect gate="-P1" pin="10" pad="B14"/>
<connect gate="-P1" pin="11" pad="C14"/>
<connect gate="-P1" pin="12" pad="F13"/>
<connect gate="-P1" pin="13" pad="E14"/>
<connect gate="-P1" pin="14" pad="D14"/>
<connect gate="-P1" pin="15" pad="F14"/>
<connect gate="-P1" pin="2" pad="D12"/>
<connect gate="-P1" pin="3" pad="B12"/>
<connect gate="-P1" pin="4" pad="C11"/>
<connect gate="-P1" pin="5" pad="C13"/>
<connect gate="-P1" pin="6" pad="A12"/>
<connect gate="-P1" pin="7" pad="B13"/>
<connect gate="-P1" pin="8" pad="A13"/>
<connect gate="-P1" pin="9" pad="A14"/>
<connect gate="-P2" pin="0" pad="P12"/>
<connect gate="-P2" pin="1" pad="P11"/>
<connect gate="-P2" pin="10" pad="L13"/>
<connect gate="-P2" pin="11" pad="G16"/>
<connect gate="-P2" pin="12" pad="K15"/>
<connect gate="-P2" pin="13" pad="K14"/>
<connect gate="-P2" pin="14" pad="F16"/>
<connect gate="-P2" pin="15" pad="E16"/>
<connect gate="-P2" pin="2" pad="P13"/>
<connect gate="-P2" pin="3" pad="P14"/>
<connect gate="-P2" pin="4" pad="N15"/>
<connect gate="-P2" pin="5" pad="N14"/>
<connect gate="-P2" pin="6" pad="N12"/>
<connect gate="-P2" pin="7" pad="K16"/>
<connect gate="-P2" pin="8" pad="J16"/>
<connect gate="-P2" pin="9" pad="H16"/>
<connect gate="-P3" pin="0" pad="A15"/>
<connect gate="-P3" pin="1" pad="B15"/>
<connect gate="-P3" pin="10" pad="B16"/>
<connect gate="-P3" pin="11" pad="C16"/>
<connect gate="-P3" pin="12" pad="D16"/>
<connect gate="-P3" pin="13" pad="K13"/>
<connect gate="-P3" pin="14" pad="J14"/>
<connect gate="-P3" pin="15" pad="J15"/>
<connect gate="-P3" pin="2" pad="D15"/>
<connect gate="-P3" pin="3" pad="E15"/>
<connect gate="-P3" pin="4" pad="G14"/>
<connect gate="-P3" pin="5" pad="G15"/>
<connect gate="-P3" pin="6" pad="F15"/>
<connect gate="-P3" pin="7" pad="H14"/>
<connect gate="-P3" pin="8" pad="C15"/>
<connect gate="-P3" pin="9" pad="H15"/>
<connect gate="-P4" pin="0" pad="R8"/>
<connect gate="-P4" pin="1" pad="R9"/>
<connect gate="-P4" pin="2" pad="N7"/>
<connect gate="-P4" pin="3" pad="N6"/>
<connect gate="-P4" pin="4" pad="P6"/>
<connect gate="-P4" pin="5" pad="R7"/>
<connect gate="-P4" pin="6" pad="R6"/>
<connect gate="-P4" pin="7" pad="P5"/>
<connect gate="-VDD1" pin="VDD" pad="G7"/>
<connect gate="-VDD2" pin="VDD" pad="G8"/>
<connect gate="-VDD3" pin="VDD" pad="G9"/>
<connect gate="-VDD4" pin="VDD" pad="G10"/>
<connect gate="-VDD5" pin="VDD" pad="G13"/>
<connect gate="-VDD6" pin="VDD" pad="K7"/>
<connect gate="-VDD7" pin="VDD" pad="K8"/>
<connect gate="-VDD8" pin="VDD" pad="K9"/>
<connect gate="-VDD9" pin="VDD" pad="K10"/>
<connect gate="-VDDP1" pin="VDDP" pad="D4"/>
<connect gate="-VDDP2" pin="VDDP" pad="D13"/>
<connect gate="-VDDP3" pin="VDDP" pad="H4"/>
<connect gate="-VDDP4" pin="VDDP" pad="J13"/>
<connect gate="-VDDP5" pin="VDDP" pad="M4"/>
<connect gate="-VDDP6" pin="VDDP" pad="N13"/>
<connect gate="-VSS1" pin="VSS" pad="E4"/>
<connect gate="-VSS10" pin="VSS" pad="J8"/>
<connect gate="-VSS11" pin="VSS" pad="J9"/>
<connect gate="-VSS12" pin="VSS" pad="J10"/>
<connect gate="-VSS13" pin="VSS" pad="M13"/>
<connect gate="-VSS14" pin="VSS" pad="N4"/>
<connect gate="-VSS15" pin="VSS" pad="R2"/>
<connect gate="-VSS16" pin="VSS" pad="T2"/>
<connect gate="-VSS2" pin="VSS" pad="E13"/>
<connect gate="-VSS3" pin="VSS" pad="H7"/>
<connect gate="-VSS4" pin="VSS" pad="H8"/>
<connect gate="-VSS5" pin="VSS" pad="H9"/>
<connect gate="-VSS6" pin="VSS" pad="H10"/>
<connect gate="-VSS7" pin="VSS" pad="H13"/>
<connect gate="-VSS8" pin="VSS" pad="J4"/>
<connect gate="-VSS9" pin="VSS" pad="J7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1130" prefix="IC">
<description>&lt;b&gt; 32-Bit Industrial &amp;Communication Controller&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. TC1130_DS_v031.pdf</description>
<gates>
<gate name="G" symbol="TC1130"/>
<gate name="PWR" symbol="PWR_TC1130"/>
<gate name="P0" symbol="PORT16"/>
<gate name="P1" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="P3" symbol="PORT16"/>
<gate name="RES" symbol="NC4"/>
</gates>
<devices>
<device name="" package="P-LBGA-208-2">
<connects>
<connect gate="G" pin="/ADV" pad="B11"/>
<connect gate="G" pin="/BAA" pad="A11"/>
<connect gate="G" pin="/BRKIN" pad="T5"/>
<connect gate="G" pin="/CAS" pad="D5"/>
<connect gate="G" pin="/CSCOMB" pad="N3"/>
<connect gate="G" pin="/HDRST" pad="N5"/>
<connect gate="G" pin="/MR_W" pad="P3"/>
<connect gate="G" pin="/PORST" pad="R5"/>
<connect gate="G" pin="/RAS" pad="D6"/>
<connect gate="G" pin="/RD" pad="P2"/>
<connect gate="G" pin="/WAIT" pad="B9"/>
<connect gate="G" pin="/WR" pad="T3"/>
<connect gate="G" pin="A0" pad="K1"/>
<connect gate="G" pin="A1" pad="L1"/>
<connect gate="G" pin="A10" pad="J3"/>
<connect gate="G" pin="A11" pad="K3"/>
<connect gate="G" pin="A12" pad="L3"/>
<connect gate="G" pin="A13" pad="M3"/>
<connect gate="G" pin="A14" pad="K4"/>
<connect gate="G" pin="A15" pad="A8"/>
<connect gate="G" pin="A16" pad="A9"/>
<connect gate="G" pin="A17" pad="A10"/>
<connect gate="G" pin="A18" pad="B10"/>
<connect gate="G" pin="A19" pad="C10"/>
<connect gate="G" pin="A2" pad="M1"/>
<connect gate="G" pin="A20" pad="D10"/>
<connect gate="G" pin="A21" pad="T4"/>
<connect gate="G" pin="A22" pad="R4"/>
<connect gate="G" pin="A23" pad="P4"/>
<connect gate="G" pin="A3" pad="N1"/>
<connect gate="G" pin="A4" pad="P1"/>
<connect gate="G" pin="A5" pad="J2"/>
<connect gate="G" pin="A6" pad="K2"/>
<connect gate="G" pin="A7" pad="L2"/>
<connect gate="G" pin="A8" pad="M2"/>
<connect gate="G" pin="A9" pad="N2"/>
<connect gate="G" pin="AD0" pad="C8"/>
<connect gate="G" pin="AD1" pad="C7"/>
<connect gate="G" pin="AD10" pad="F1"/>
<connect gate="G" pin="AD11" pad="E3"/>
<connect gate="G" pin="AD12" pad="F3"/>
<connect gate="G" pin="AD13" pad="G1"/>
<connect gate="G" pin="AD14" pad="H2"/>
<connect gate="G" pin="AD15" pad="G3"/>
<connect gate="G" pin="AD16" pad="D7"/>
<connect gate="G" pin="AD17" pad="B5"/>
<connect gate="G" pin="AD18" pad="A4"/>
<connect gate="G" pin="AD19" pad="B4"/>
<connect gate="G" pin="AD2" pad="B6"/>
<connect gate="G" pin="AD20" pad="C4"/>
<connect gate="G" pin="AD21" pad="B3"/>
<connect gate="G" pin="AD22" pad="B2"/>
<connect gate="G" pin="AD23" pad="B1"/>
<connect gate="G" pin="AD24" pad="C1"/>
<connect gate="G" pin="AD25" pad="D3"/>
<connect gate="G" pin="AD26" pad="E2"/>
<connect gate="G" pin="AD27" pad="F2"/>
<connect gate="G" pin="AD28" pad="F4"/>
<connect gate="G" pin="AD29" pad="G4"/>
<connect gate="G" pin="AD3" pad="C6"/>
<connect gate="G" pin="AD30" pad="H3"/>
<connect gate="G" pin="AD31" pad="G2"/>
<connect gate="G" pin="AD4" pad="C5"/>
<connect gate="G" pin="AD5" pad="A3"/>
<connect gate="G" pin="AD6" pad="A2"/>
<connect gate="G" pin="AD7" pad="C3"/>
<connect gate="G" pin="AD8" pad="C2"/>
<connect gate="G" pin="AD9" pad="D2"/>
<connect gate="G" pin="ALE" pad="R3"/>
<connect gate="G" pin="BC0" pad="A5"/>
<connect gate="G" pin="BC1" pad="A6"/>
<connect gate="G" pin="BC2" pad="B7"/>
<connect gate="G" pin="BC3" pad="A7"/>
<connect gate="G" pin="BFCLKI" pad="D1"/>
<connect gate="G" pin="BFCLKO" pad="E1"/>
<connect gate="G" pin="CKE" pad="L4"/>
<connect gate="G" pin="CS0" pad="D9"/>
<connect gate="G" pin="CS1" pad="D8"/>
<connect gate="G" pin="CS2" pad="C9"/>
<connect gate="G" pin="CS3" pad="B8"/>
<connect gate="G" pin="D+" pad="T14"/>
<connect gate="G" pin="D-" pad="T15"/>
<connect gate="G" pin="HWCFG0" pad="M14"/>
<connect gate="G" pin="HWCFG1" pad="L14"/>
<connect gate="G" pin="HWCFG2" pad="T6"/>
<connect gate="G" pin="MI_MDIO" pad="R1"/>
<connect gate="G" pin="MI_RXCLK" pad="R2"/>
<connect gate="G" pin="MI_TXCLK" pad="T2"/>
<connect gate="G" pin="NMI" pad="T7"/>
<connect gate="G" pin="P4.0" pad="R8"/>
<connect gate="G" pin="P4.1" pad="R9"/>
<connect gate="G" pin="P4.2" pad="N7"/>
<connect gate="G" pin="P4.3" pad="N6"/>
<connect gate="G" pin="P4.4" pad="P6"/>
<connect gate="G" pin="P4.5" pad="R7"/>
<connect gate="G" pin="P4.6" pad="R6"/>
<connect gate="G" pin="P4.7" pad="P5"/>
<connect gate="G" pin="SDCLKI" pad="J1"/>
<connect gate="G" pin="SDCLKO" pad="H1"/>
<connect gate="G" pin="TCK" pad="T12"/>
<connect gate="G" pin="TDI" pad="T13"/>
<connect gate="G" pin="TDO" pad="T10"/>
<connect gate="G" pin="TMS" pad="T9"/>
<connect gate="G" pin="TRCLK" pad="T8"/>
<connect gate="G" pin="TRST" pad="T11"/>
<connect gate="G" pin="VDDOSC" pad="L16"/>
<connect gate="G" pin="VDDOSC3" pad="P16"/>
<connect gate="G" pin="VSSOSC" pad="N4"/>
<connect gate="G" pin="VSSOSC3" pad="R16"/>
<connect gate="G" pin="XTAL1" pad="M16"/>
<connect gate="G" pin="XTAL2" pad="N16"/>
<connect gate="P0" pin="0" pad="N11"/>
<connect gate="P0" pin="1" pad="P15"/>
<connect gate="P0" pin="10" pad="R14"/>
<connect gate="P0" pin="11" pad="N9"/>
<connect gate="P0" pin="12" pad="P9"/>
<connect gate="P0" pin="13" pad="P8"/>
<connect gate="P0" pin="14" pad="N8"/>
<connect gate="P0" pin="15" pad="P7"/>
<connect gate="P0" pin="2" pad="P10"/>
<connect gate="P0" pin="3" pad="M15"/>
<connect gate="P0" pin="4" pad="R11"/>
<connect gate="P0" pin="5" pad="R12"/>
<connect gate="P0" pin="6" pad="R10"/>
<connect gate="P0" pin="7" pad="N10"/>
<connect gate="P0" pin="8" pad="R13"/>
<connect gate="P0" pin="9" pad="R15"/>
<connect gate="P1" pin="0" pad="D11"/>
<connect gate="P1" pin="1" pad="C12"/>
<connect gate="P1" pin="10" pad="B14"/>
<connect gate="P1" pin="11" pad="C14"/>
<connect gate="P1" pin="12" pad="F13"/>
<connect gate="P1" pin="13" pad="E14"/>
<connect gate="P1" pin="14" pad="D14"/>
<connect gate="P1" pin="15" pad="F14"/>
<connect gate="P1" pin="2" pad="D12"/>
<connect gate="P1" pin="3" pad="B12"/>
<connect gate="P1" pin="4" pad="C11"/>
<connect gate="P1" pin="5" pad="C13"/>
<connect gate="P1" pin="6" pad="A12"/>
<connect gate="P1" pin="7" pad="B13"/>
<connect gate="P1" pin="8" pad="A13"/>
<connect gate="P1" pin="9" pad="A14"/>
<connect gate="P2" pin="0" pad="P12"/>
<connect gate="P2" pin="1" pad="P11"/>
<connect gate="P2" pin="10" pad="L13"/>
<connect gate="P2" pin="11" pad="G16"/>
<connect gate="P2" pin="12" pad="K15"/>
<connect gate="P2" pin="13" pad="K14"/>
<connect gate="P2" pin="14" pad="F16"/>
<connect gate="P2" pin="15" pad="E16"/>
<connect gate="P2" pin="2" pad="P13"/>
<connect gate="P2" pin="3" pad="P14"/>
<connect gate="P2" pin="4" pad="N15"/>
<connect gate="P2" pin="5" pad="N14"/>
<connect gate="P2" pin="6" pad="N12"/>
<connect gate="P2" pin="7" pad="K16"/>
<connect gate="P2" pin="8" pad="J16"/>
<connect gate="P2" pin="9" pad="H16"/>
<connect gate="P3" pin="0" pad="A15"/>
<connect gate="P3" pin="1" pad="B15"/>
<connect gate="P3" pin="10" pad="B16"/>
<connect gate="P3" pin="11" pad="C16"/>
<connect gate="P3" pin="12" pad="D16"/>
<connect gate="P3" pin="13" pad="K13"/>
<connect gate="P3" pin="14" pad="J14"/>
<connect gate="P3" pin="15" pad="J15"/>
<connect gate="P3" pin="2" pad="D15"/>
<connect gate="P3" pin="3" pad="E15"/>
<connect gate="P3" pin="4" pad="G14"/>
<connect gate="P3" pin="5" pad="G15"/>
<connect gate="P3" pin="6" pad="F15"/>
<connect gate="P3" pin="7" pad="H14"/>
<connect gate="P3" pin="8" pad="C15"/>
<connect gate="P3" pin="9" pad="H15"/>
<connect gate="PWR" pin="VDD@0" pad="G7"/>
<connect gate="PWR" pin="VDD@1" pad="G8"/>
<connect gate="PWR" pin="VDD@2" pad="G9"/>
<connect gate="PWR" pin="VDD@3" pad="G10"/>
<connect gate="PWR" pin="VDD@4" pad="G13"/>
<connect gate="PWR" pin="VDD@5" pad="K7"/>
<connect gate="PWR" pin="VDD@6" pad="K8"/>
<connect gate="PWR" pin="VDD@7" pad="K9"/>
<connect gate="PWR" pin="VDD@8" pad="K10"/>
<connect gate="PWR" pin="VDDP@0" pad="D4"/>
<connect gate="PWR" pin="VDDP@1" pad="D13"/>
<connect gate="PWR" pin="VDDP@2" pad="H4"/>
<connect gate="PWR" pin="VDDP@3" pad="J13"/>
<connect gate="PWR" pin="VDDP@4" pad="M4"/>
<connect gate="PWR" pin="VDDP@5" pad="N13"/>
<connect gate="PWR" pin="VSS@0" pad="E4"/>
<connect gate="PWR" pin="VSS@1" pad="E13"/>
<connect gate="PWR" pin="VSS@10" pad="J9"/>
<connect gate="PWR" pin="VSS@11" pad="J10"/>
<connect gate="PWR" pin="VSS@12" pad="L15"/>
<connect gate="PWR" pin="VSS@13" pad="M13"/>
<connect gate="PWR" pin="VSS@2" pad="H7"/>
<connect gate="PWR" pin="VSS@3" pad="H8"/>
<connect gate="PWR" pin="VSS@4" pad="H9"/>
<connect gate="PWR" pin="VSS@5" pad="H10"/>
<connect gate="PWR" pin="VSS@6" pad="H13"/>
<connect gate="PWR" pin="VSS@7" pad="J4"/>
<connect gate="PWR" pin="VSS@8" pad="J7"/>
<connect gate="PWR" pin="VSS@9" pad="J8"/>
<connect gate="RES" pin="RESERVED@0" pad="A1"/>
<connect gate="RES" pin="RESERVED@1" pad="A16"/>
<connect gate="RES" pin="RESERVED@2" pad="T1"/>
<connect gate="RES" pin="RESERVED@3" pad="T16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1762" prefix="IC">
<description>Infineon TriCore NG (Next Generation) 32bit Microcontroller/DSP</description>
<gates>
<gate name="G" symbol="TC1762"/>
<gate name="PWR" symbol="PWR_TC1762"/>
</gates>
<devices>
<device name="" package="P-LQFP-176-2">
<connects>
<connect gate="G" pin="/BRKIN" pad="117"/>
<connect gate="G" pin="/BRKOUT" pad="116"/>
<connect gate="G" pin="/HDRST" pad="122"/>
<connect gate="G" pin="/NMI" pad="120"/>
<connect gate="G" pin="/PORST" pad="121"/>
<connect gate="G" pin="/TEST_MODE" pad="118"/>
<connect gate="G" pin="/TRST" pad="114"/>
<connect gate="G" pin="AN0" pad="67"/>
<connect gate="G" pin="AN1" pad="66"/>
<connect gate="G" pin="AN10" pad="58"/>
<connect gate="G" pin="AN11" pad="57"/>
<connect gate="G" pin="AN12" pad="56"/>
<connect gate="G" pin="AN13" pad="55"/>
<connect gate="G" pin="AN14" pad="50"/>
<connect gate="G" pin="AN15" pad="49"/>
<connect gate="G" pin="AN16" pad="48"/>
<connect gate="G" pin="AN17" pad="47"/>
<connect gate="G" pin="AN18" pad="46"/>
<connect gate="G" pin="AN19" pad="45"/>
<connect gate="G" pin="AN2" pad="65"/>
<connect gate="G" pin="AN20" pad="44"/>
<connect gate="G" pin="AN21" pad="43"/>
<connect gate="G" pin="AN22" pad="42"/>
<connect gate="G" pin="AN23" pad="41"/>
<connect gate="G" pin="AN24" pad="40"/>
<connect gate="G" pin="AN25" pad="39"/>
<connect gate="G" pin="AN26" pad="38"/>
<connect gate="G" pin="AN27" pad="37"/>
<connect gate="G" pin="AN28" pad="35"/>
<connect gate="G" pin="AN29" pad="34"/>
<connect gate="G" pin="AN3" pad="64"/>
<connect gate="G" pin="AN30" pad="33"/>
<connect gate="G" pin="AN31" pad="32"/>
<connect gate="G" pin="AN32" pad="31"/>
<connect gate="G" pin="AN33" pad="30"/>
<connect gate="G" pin="AN34" pad="29"/>
<connect gate="G" pin="AN35" pad="28"/>
<connect gate="G" pin="AN4" pad="63"/>
<connect gate="G" pin="AN5" pad="62"/>
<connect gate="G" pin="AN6" pad="61"/>
<connect gate="G" pin="AN7" pad="36"/>
<connect gate="G" pin="AN8" pad="60"/>
<connect gate="G" pin="AN9" pad="59"/>
<connect gate="G" pin="BYPASS" pad="119"/>
<connect gate="G" pin="FCLN0" pad="156"/>
<connect gate="G" pin="FCLP0A" pad="157"/>
<connect gate="G" pin="NC@0" pad="21"/>
<connect gate="G" pin="NC@1" pad="89"/>
<connect gate="G" pin="P0.0" pad="145"/>
<connect gate="G" pin="P0.1" pad="146"/>
<connect gate="G" pin="P0.10" pad="151"/>
<connect gate="G" pin="P0.11" pad="152"/>
<connect gate="G" pin="P0.12" pad="168"/>
<connect gate="G" pin="P0.13" pad="169"/>
<connect gate="G" pin="P0.14" pad="175"/>
<connect gate="G" pin="P0.15" pad="176"/>
<connect gate="G" pin="P0.2" pad="147"/>
<connect gate="G" pin="P0.3" pad="148"/>
<connect gate="G" pin="P0.4" pad="166"/>
<connect gate="G" pin="P0.5" pad="167"/>
<connect gate="G" pin="P0.6" pad="173"/>
<connect gate="G" pin="P0.7" pad="174"/>
<connect gate="G" pin="P0.8" pad="149"/>
<connect gate="G" pin="P0.9" pad="150"/>
<connect gate="G" pin="P1.0" pad="91"/>
<connect gate="G" pin="P1.1" pad="92"/>
<connect gate="G" pin="P1.10" pad="96"/>
<connect gate="G" pin="P1.11" pad="97"/>
<connect gate="G" pin="P1.12" pad="73"/>
<connect gate="G" pin="P1.13" pad="72"/>
<connect gate="G" pin="P1.14" pad="71"/>
<connect gate="G" pin="P1.2" pad="93"/>
<connect gate="G" pin="P1.3" pad="98"/>
<connect gate="G" pin="P1.4" pad="107"/>
<connect gate="G" pin="P1.5" pad="108"/>
<connect gate="G" pin="P1.6" pad="109"/>
<connect gate="G" pin="P1.7" pad="110"/>
<connect gate="G" pin="P1.8" pad="94"/>
<connect gate="G" pin="P1.9" pad="95"/>
<connect gate="G" pin="P2.0" pad="74"/>
<connect gate="G" pin="P2.1" pad="75"/>
<connect gate="G" pin="P2.10" pad="161"/>
<connect gate="G" pin="P2.11" pad="162"/>
<connect gate="G" pin="P2.12" pad="163"/>
<connect gate="G" pin="P2.13" pad="165"/>
<connect gate="G" pin="P2.2" pad="76"/>
<connect gate="G" pin="P2.3" pad="77"/>
<connect gate="G" pin="P2.4" pad="78"/>
<connect gate="G" pin="P2.5" pad="79"/>
<connect gate="G" pin="P2.6" pad="80"/>
<connect gate="G" pin="P2.7" pad="81"/>
<connect gate="G" pin="P2.8" pad="164"/>
<connect gate="G" pin="P2.9" pad="160"/>
<connect gate="G" pin="P3.0" pad="136"/>
<connect gate="G" pin="P3.1" pad="135"/>
<connect gate="G" pin="P3.10" pad="137"/>
<connect gate="G" pin="P3.11" pad="144"/>
<connect gate="G" pin="P3.12" pad="143"/>
<connect gate="G" pin="P3.13" pad="142"/>
<connect gate="G" pin="P3.14" pad="134"/>
<connect gate="G" pin="P3.15" pad="133"/>
<connect gate="G" pin="P3.2" pad="129"/>
<connect gate="G" pin="P3.3" pad="130"/>
<connect gate="G" pin="P3.4" pad="132"/>
<connect gate="G" pin="P3.5" pad="126"/>
<connect gate="G" pin="P3.6" pad="127"/>
<connect gate="G" pin="P3.7" pad="131"/>
<connect gate="G" pin="P3.8" pad="128"/>
<connect gate="G" pin="P3.9" pad="138"/>
<connect gate="G" pin="P4.0" pad="86"/>
<connect gate="G" pin="P4.1" pad="87"/>
<connect gate="G" pin="P4.2" pad="88"/>
<connect gate="G" pin="P4.3" pad="90"/>
<connect gate="G" pin="P5.0" pad="1"/>
<connect gate="G" pin="P5.1" pad="2"/>
<connect gate="G" pin="P5.10" pad="15"/>
<connect gate="G" pin="P5.11" pad="16"/>
<connect gate="G" pin="P5.12" pad="17"/>
<connect gate="G" pin="P5.13" pad="18"/>
<connect gate="G" pin="P5.14" pad="19"/>
<connect gate="G" pin="P5.15" pad="20"/>
<connect gate="G" pin="P5.2" pad="3"/>
<connect gate="G" pin="P5.3" pad="4"/>
<connect gate="G" pin="P5.4" pad="5"/>
<connect gate="G" pin="P5.5" pad="6"/>
<connect gate="G" pin="P5.6" pad="7"/>
<connect gate="G" pin="P5.7" pad="8"/>
<connect gate="G" pin="P5.8" pad="13"/>
<connect gate="G" pin="P5.9" pad="14"/>
<connect gate="G" pin="SON0" pad="158"/>
<connect gate="G" pin="SOP0A" pad="159"/>
<connect gate="G" pin="TCK" pad="115"/>
<connect gate="G" pin="TDI" pad="111"/>
<connect gate="G" pin="TDO" pad="113"/>
<connect gate="G" pin="TMS" pad="112"/>
<connect gate="G" pin="TRCLK" pad="9"/>
<connect gate="G" pin="XTAL1" pad="102"/>
<connect gate="G" pin="XTAL2" pad="103"/>
<connect gate="PWR" pin="VAGND" pad="27"/>
<connect gate="PWR" pin="VAGND0" pad="51"/>
<connect gate="PWR" pin="VAREF" pad="26"/>
<connect gate="PWR" pin="VAREF0" pad="52"/>
<connect gate="PWR" pin="VDD@0" pad="10"/>
<connect gate="PWR" pin="VDD@1" pad="68"/>
<connect gate="PWR" pin="VDD@2" pad="84"/>
<connect gate="PWR" pin="VDD@3" pad="99"/>
<connect gate="PWR" pin="VDD@4" pad="123"/>
<connect gate="PWR" pin="VDD@5" pad="153"/>
<connect gate="PWR" pin="VDD@6" pad="170"/>
<connect gate="PWR" pin="VDDAF" pad="23"/>
<connect gate="PWR" pin="VDDFL3" pad="141"/>
<connect gate="PWR" pin="VDDM" pad="54"/>
<connect gate="PWR" pin="VDDMF" pad="24"/>
<connect gate="PWR" pin="VDDOSC" pad="105"/>
<connect gate="PWR" pin="VDDOSC3" pad="106"/>
<connect gate="PWR" pin="VDDP@0" pad="11"/>
<connect gate="PWR" pin="VDDP@1" pad="69"/>
<connect gate="PWR" pin="VDDP@2" pad="83"/>
<connect gate="PWR" pin="VDDP@3" pad="100"/>
<connect gate="PWR" pin="VDDP@4" pad="124"/>
<connect gate="PWR" pin="VDDP@5" pad="154"/>
<connect gate="PWR" pin="VDDP@6" pad="171"/>
<connect gate="PWR" pin="VDDP@7" pad="139"/>
<connect gate="PWR" pin="VSS@0" pad="12"/>
<connect gate="PWR" pin="VSS@1" pad="70"/>
<connect gate="PWR" pin="VSS@2" pad="85"/>
<connect gate="PWR" pin="VSS@3" pad="101"/>
<connect gate="PWR" pin="VSS@4" pad="125"/>
<connect gate="PWR" pin="VSS@5" pad="155"/>
<connect gate="PWR" pin="VSS@6" pad="172"/>
<connect gate="PWR" pin="VSS@7" pad="140"/>
<connect gate="PWR" pin="VSS@8" pad="82"/>
<connect gate="PWR" pin="VSSAF" pad="22"/>
<connect gate="PWR" pin="VSSM" pad="53"/>
<connect gate="PWR" pin="VSSMF" pad="25"/>
<connect gate="PWR" pin="VSSOSC" pad="104"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1765" prefix="IC">
<description>&lt;b&gt;TC1765 (AUDO1)&lt;/b&gt; 32-bit microcontroller&lt;p&gt;
for automotive and industrial applications &lt;br&gt;
(e.g. engine management, transmission, starter generator or 3-phase motor control)&lt;br&gt;
Source: http://www.infineon.com ..</description>
<gates>
<gate name="TP" symbol="PORT16"/>
<gate name="D" symbol="D31"/>
<gate name="A" symbol="A23"/>
<gate name="AN" symbol="AN23"/>
<gate name="JTAG" symbol="JTAG-OCSD"/>
<gate name="P1" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="P3" symbol="PORT16"/>
<gate name="P0" symbol="PORT16"/>
<gate name="PW1" symbol="VSS_VDD"/>
<gate name="PW2" symbol="VSS_VDD"/>
<gate name="PW3" symbol="VSS_VDD"/>
<gate name="PW4" symbol="VSS_VDD"/>
<gate name="PW5" symbol="VSS_VDD"/>
<gate name="PW6" symbol="VSS_VDD"/>
<gate name="PW7" symbol="VSS_VDD"/>
<gate name="PW8" symbol="VSS_VDD"/>
<gate name="PW9" symbol="VSS_VDD"/>
<gate name="PW10" symbol="VSS_VDD"/>
<gate name="G" symbol="TC1765"/>
<gate name="AREF0" symbol="VSS_VDD"/>
<gate name="AREF1" symbol="VSS_VDD"/>
<gate name="PW11" symbol="VSS_VDD"/>
<gate name="PW12" symbol="VSS_VDD"/>
<gate name="PW13" symbol="VSS_VDD"/>
<gate name="PW14" symbol="VSS_VDD"/>
<gate name="PW15" symbol="VSS_VDD"/>
<gate name="PW16" symbol="VSS_VDD"/>
<gate name="PW17" symbol="VSS_VDD"/>
<gate name="PW18" symbol="VSS_VDD"/>
<gate name="PW19" symbol="VSS_VDD"/>
<gate name="PW20" symbol="VSS_VDD"/>
<gate name="PW21" symbol="VSS_VDD"/>
<gate name="PW23" symbol="GND6"/>
</gates>
<devices>
<device name="" package="P-LBGA-260">
<connects>
<connect gate="A" pin="A0" pad="T5"/>
<connect gate="A" pin="A1" pad="V4"/>
<connect gate="A" pin="A10" pad="U7"/>
<connect gate="A" pin="A11" pad="T7"/>
<connect gate="A" pin="A12" pad="V8"/>
<connect gate="A" pin="A13" pad="U14"/>
<connect gate="A" pin="A14" pad="U8"/>
<connect gate="A" pin="A15" pad="T8"/>
<connect gate="A" pin="A16" pad="T9"/>
<connect gate="A" pin="A17" pad="V14"/>
<connect gate="A" pin="A18" pad="U9"/>
<connect gate="A" pin="A19" pad="R9"/>
<connect gate="A" pin="A2" pad="U5"/>
<connect gate="A" pin="A20" pad="V13"/>
<connect gate="A" pin="A21" pad="T11"/>
<connect gate="A" pin="A22" pad="V10"/>
<connect gate="A" pin="A23" pad="U10"/>
<connect gate="A" pin="A3" pad="R6"/>
<connect gate="A" pin="A4" pad="V5"/>
<connect gate="A" pin="A5" pad="R7"/>
<connect gate="A" pin="A6" pad="T6"/>
<connect gate="A" pin="A7" pad="U6"/>
<connect gate="A" pin="A8" pad="R8"/>
<connect gate="A" pin="A9" pad="V6"/>
<connect gate="AN" pin="AN0" pad="A7"/>
<connect gate="AN" pin="AN1" pad="D6"/>
<connect gate="AN" pin="AN10" pad="C3"/>
<connect gate="AN" pin="AN11" pad="B3"/>
<connect gate="AN" pin="AN12" pad="D3"/>
<connect gate="AN" pin="AN13" pad="D4"/>
<connect gate="AN" pin="AN14" pad="E4"/>
<connect gate="AN" pin="AN15" pad="E3"/>
<connect gate="AN" pin="AN16" pad="A2"/>
<connect gate="AN" pin="AN17" pad="A1"/>
<connect gate="AN" pin="AN18" pad="B2"/>
<connect gate="AN" pin="AN19" pad="B1"/>
<connect gate="AN" pin="AN2" pad="B6"/>
<connect gate="AN" pin="AN20" pad="C2"/>
<connect gate="AN" pin="AN21" pad="F4"/>
<connect gate="AN" pin="AN22" pad="F3"/>
<connect gate="AN" pin="AN23" pad="D2"/>
<connect gate="AN" pin="AN3" pad="D5"/>
<connect gate="AN" pin="AN4" pad="A6"/>
<connect gate="AN" pin="AN5" pad="B5"/>
<connect gate="AN" pin="AN6" pad="C5"/>
<connect gate="AN" pin="AN7" pad="A5"/>
<connect gate="AN" pin="AN8" pad="A3"/>
<connect gate="AN" pin="AN9" pad="C4"/>
<connect gate="AREF0" pin="VDD" pad="C1"/>
<connect gate="AREF0" pin="VSS" pad="E2"/>
<connect gate="AREF1" pin="VDD" pad="A8"/>
<connect gate="AREF1" pin="VSS" pad="C6"/>
<connect gate="D" pin="D0" pad="T3"/>
<connect gate="D" pin="D1" pad="R4"/>
<connect gate="D" pin="D10" pad="L4"/>
<connect gate="D" pin="D11" pad="M3"/>
<connect gate="D" pin="D12" pad="N2"/>
<connect gate="D" pin="D13" pad="M2"/>
<connect gate="D" pin="D14" pad="L3"/>
<connect gate="D" pin="D15" pad="M1"/>
<connect gate="D" pin="D16" pad="L1"/>
<connect gate="D" pin="D17" pad="K1"/>
<connect gate="D" pin="D18" pad="K2"/>
<connect gate="D" pin="D19" pad="K3"/>
<connect gate="D" pin="D2" pad="P4"/>
<connect gate="D" pin="D20" pad="J1"/>
<connect gate="D" pin="D21" pad="J2"/>
<connect gate="D" pin="D22" pad="H2"/>
<connect gate="D" pin="D23" pad="H1"/>
<connect gate="D" pin="D24" pad="J4"/>
<connect gate="D" pin="D25" pad="H3"/>
<connect gate="D" pin="D26" pad="G2"/>
<connect gate="D" pin="D27" pad="G1"/>
<connect gate="D" pin="D28" pad="F1"/>
<connect gate="D" pin="D29" pad="E1"/>
<connect gate="D" pin="D3" pad="R2"/>
<connect gate="D" pin="D30" pad="F2"/>
<connect gate="D" pin="D31" pad="H4"/>
<connect gate="D" pin="D4" pad="R1"/>
<connect gate="D" pin="D5" pad="R3"/>
<connect gate="D" pin="D6" pad="N4"/>
<connect gate="D" pin="D7" pad="P3"/>
<connect gate="D" pin="D8" pad="M4"/>
<connect gate="D" pin="D9" pad="N3"/>
<connect gate="G" pin="/BAA" pad="U4"/>
<connect gate="G" pin="/BC0" pad="U2"/>
<connect gate="G" pin="/BC1" pad="V1"/>
<connect gate="G" pin="/BC2" pad="U3"/>
<connect gate="G" pin="/BC3" pad="V2"/>
<connect gate="G" pin="/CDEMU/!CSOVK" pad="V11"/>
<connect gate="G" pin="/CODE" pad="V3"/>
<connect gate="G" pin="/CS0" pad="U12"/>
<connect gate="G" pin="/CS1" pad="V12"/>
<connect gate="G" pin="/CS2" pad="T10"/>
<connect gate="G" pin="/CS3" pad="R10"/>
<connect gate="G" pin="/HDRST" pad="P18"/>
<connect gate="G" pin="/NMI" pad="U17"/>
<connect gate="G" pin="/PO_RST" pad="T17"/>
<connect gate="G" pin="/TEST/MODE" pad="V16"/>
<connect gate="G" pin="/WAIT/!IND" pad="R5"/>
<connect gate="G" pin="ADV" pad="U1"/>
<connect gate="G" pin="BYPASS" pad="N17"/>
<connect gate="G" pin="CPUCLK" pad="R13"/>
<connect gate="G" pin="ECIN" pad="N1"/>
<connect gate="G" pin="ECOUT" pad="P1"/>
<connect gate="G" pin="NC@0" pad="V17"/>
<connect gate="G" pin="NC@1" pad="V18"/>
<connect gate="G" pin="P4.0" pad="D14"/>
<connect gate="G" pin="P4.1" pad="C13"/>
<connect gate="G" pin="P4.2" pad="A17"/>
<connect gate="G" pin="P4.3" pad="B15"/>
<connect gate="G" pin="P4.4" pad="C16"/>
<connect gate="G" pin="P4.5" pad="D13"/>
<connect gate="G" pin="P4.6" pad="C15"/>
<connect gate="G" pin="P4.7" pad="C12"/>
<connect gate="G" pin="P5.0" pad="D12"/>
<connect gate="G" pin="P5.1" pad="B13"/>
<connect gate="G" pin="P5.2" pad="B14"/>
<connect gate="G" pin="P5.3" pad="C11"/>
<connect gate="G" pin="P5.4" pad="A16"/>
<connect gate="G" pin="RD" pad="T1"/>
<connect gate="G" pin="RD/!WR" pad="T2"/>
<connect gate="G" pin="XTAL1" pad="U18"/>
<connect gate="G" pin="XTAL2" pad="T18"/>
<connect gate="JTAG" pin="!BRKIN" pad="U15"/>
<connect gate="JTAG" pin="!BRKOUT" pad="T12"/>
<connect gate="JTAG" pin="!OCDSE" pad="R11"/>
<connect gate="JTAG" pin="!TRST" pad="R14"/>
<connect gate="JTAG" pin="TCK" pad="T13"/>
<connect gate="JTAG" pin="TDI" pad="T14"/>
<connect gate="JTAG" pin="TDO" pad="R12"/>
<connect gate="JTAG" pin="TMS" pad="V15"/>
<connect gate="P0" pin="0" pad="A10"/>
<connect gate="P0" pin="1" pad="D7"/>
<connect gate="P0" pin="10" pad="A14"/>
<connect gate="P0" pin="11" pad="C9"/>
<connect gate="P0" pin="12" pad="C10"/>
<connect gate="P0" pin="13" pad="D10"/>
<connect gate="P0" pin="14" pad="A15"/>
<connect gate="P0" pin="15" pad="B11"/>
<connect gate="P0" pin="2" pad="B8"/>
<connect gate="P0" pin="3" pad="C7"/>
<connect gate="P0" pin="4" pad="A11"/>
<connect gate="P0" pin="5" pad="A12"/>
<connect gate="P0" pin="6" pad="D8"/>
<connect gate="P0" pin="7" pad="B9"/>
<connect gate="P0" pin="8" pad="A13"/>
<connect gate="P0" pin="9" pad="B10"/>
<connect gate="P1" pin="0" pad="N18"/>
<connect gate="P1" pin="1" pad="R16"/>
<connect gate="P1" pin="10" pad="M16"/>
<connect gate="P1" pin="11" pad="L16"/>
<connect gate="P1" pin="12" pad="K17"/>
<connect gate="P1" pin="13" pad="K18"/>
<connect gate="P1" pin="14" pad="L15"/>
<connect gate="P1" pin="15" pad="K16"/>
<connect gate="P1" pin="2" pad="R15"/>
<connect gate="P1" pin="3" pad="M17"/>
<connect gate="P1" pin="4" pad="N16"/>
<connect gate="P1" pin="5" pad="P15"/>
<connect gate="P1" pin="6" pad="M18"/>
<connect gate="P1" pin="7" pad="L18"/>
<connect gate="P1" pin="8" pad="P16"/>
<connect gate="P1" pin="9" pad="U16"/>
<connect gate="P2" pin="0" pad="J18"/>
<connect gate="P2" pin="1" pad="T15"/>
<connect gate="P2" pin="10" pad="G18"/>
<connect gate="P2" pin="11" pad="H15"/>
<connect gate="P2" pin="12" pad="G15"/>
<connect gate="P2" pin="13" pad="G17"/>
<connect gate="P2" pin="14" pad="G16"/>
<connect gate="P2" pin="15" pad="F18"/>
<connect gate="P2" pin="2" pad="N15"/>
<connect gate="P2" pin="3" pad="J17"/>
<connect gate="P2" pin="4" pad="H18"/>
<connect gate="P2" pin="5" pad="J16"/>
<connect gate="P2" pin="6" pad="T16"/>
<connect gate="P2" pin="7" pad="M15"/>
<connect gate="P2" pin="8" pad="J15"/>
<connect gate="P2" pin="9" pad="H16"/>
<connect gate="P3" pin="0" pad="F16"/>
<connect gate="P3" pin="1" pad="F15"/>
<connect gate="P3" pin="10" pad="B18"/>
<connect gate="P3" pin="11" pad="A18"/>
<connect gate="P3" pin="12" pad="C14"/>
<connect gate="P3" pin="13" pad="D15"/>
<connect gate="P3" pin="14" pad="B17"/>
<connect gate="P3" pin="15" pad="B16"/>
<connect gate="P3" pin="2" pad="E18"/>
<connect gate="P3" pin="3" pad="E16"/>
<connect gate="P3" pin="4" pad="E15"/>
<connect gate="P3" pin="5" pad="E17"/>
<connect gate="P3" pin="6" pad="D18"/>
<connect gate="P3" pin="7" pad="D17"/>
<connect gate="P3" pin="8" pad="C18"/>
<connect gate="P3" pin="9" pad="C17"/>
<connect gate="PW1" pin="VDD" pad="J3"/>
<connect gate="PW1" pin="VSS" pad="K4"/>
<connect gate="PW10" pin="VDD" pad="C8"/>
<connect gate="PW10" pin="VSS" pad="J11"/>
<connect gate="PW11" pin="VDD" pad="A9"/>
<connect gate="PW11" pin="VSS" pad="A4"/>
<connect gate="PW12" pin="VDD" pad="B4"/>
<connect gate="PW12" pin="VSS" pad="B7"/>
<connect gate="PW13" pin="VDD" pad="B12"/>
<connect gate="PW13" pin="VSS" pad="D1"/>
<connect gate="PW14" pin="VDD" pad="D11"/>
<connect gate="PW14" pin="VSS" pad="D9"/>
<connect gate="PW15" pin="VDD" pad="D16"/>
<connect gate="PW15" pin="VSS" pad="J12"/>
<connect gate="PW16" pin="VDD" pad="G3"/>
<connect gate="PW16" pin="VSS" pad="K7"/>
<connect gate="PW17" pin="VDD" pad="G4"/>
<connect gate="PW17" pin="VSS" pad="K8"/>
<connect gate="PW18" pin="VDD" pad="H17"/>
<connect gate="PW18" pin="VSS" pad="K9"/>
<connect gate="PW19" pin="VDD" pad="R18"/>
<connect gate="PW19" pin="VSS" pad="K10"/>
<connect gate="PW2" pin="VDD" pad="L2"/>
<connect gate="PW2" pin="VSS" pad="G9"/>
<connect gate="PW20" pin="VDD" pad="P17"/>
<connect gate="PW20" pin="VSS" pad="K11"/>
<connect gate="PW21" pin="VDD" pad="L17"/>
<connect gate="PW21" pin="VSS" pad="K12"/>
<connect gate="PW23" pin="GND@0" pad="K15"/>
<connect gate="PW23" pin="GND@1" pad="L9"/>
<connect gate="PW23" pin="GND@2" pad="L10"/>
<connect gate="PW23" pin="GND@3" pad="M9"/>
<connect gate="PW23" pin="GND@4" pad="M10"/>
<connect gate="PW23" pin="GND@5" pad="R17"/>
<connect gate="PW3" pin="VDD" pad="P2"/>
<connect gate="PW3" pin="VSS" pad="G10"/>
<connect gate="PW4" pin="VDD" pad="T4"/>
<connect gate="PW4" pin="VSS" pad="H9"/>
<connect gate="PW5" pin="VDD" pad="V7"/>
<connect gate="PW5" pin="VSS" pad="H10"/>
<connect gate="PW6" pin="VDD" pad="V9"/>
<connect gate="PW6" pin="VSS" pad="J7"/>
<connect gate="PW7" pin="VDD" pad="U11"/>
<connect gate="PW7" pin="VSS" pad="J8"/>
<connect gate="PW8" pin="VDD" pad="U13"/>
<connect gate="PW8" pin="VSS" pad="J9"/>
<connect gate="PW9" pin="VDD" pad="F17"/>
<connect gate="PW9" pin="VSS" pad="J10"/>
<connect gate="TP" pin="0" pad="G7"/>
<connect gate="TP" pin="1" pad="G8"/>
<connect gate="TP" pin="10" pad="L11"/>
<connect gate="TP" pin="11" pad="L12"/>
<connect gate="TP" pin="12" pad="H11"/>
<connect gate="TP" pin="13" pad="H12"/>
<connect gate="TP" pin="14" pad="G11"/>
<connect gate="TP" pin="15" pad="G12"/>
<connect gate="TP" pin="2" pad="H7"/>
<connect gate="TP" pin="3" pad="H8"/>
<connect gate="TP" pin="4" pad="L7"/>
<connect gate="TP" pin="5" pad="L8"/>
<connect gate="TP" pin="6" pad="M7"/>
<connect gate="TP" pin="7" pad="M8"/>
<connect gate="TP" pin="8" pad="M11"/>
<connect gate="TP" pin="9" pad="M12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1775" prefix="IC">
<description>&lt;b&gt;TC1775 (AUDO1)&lt;/b&gt; 32-bit microcontroller&lt;p&gt;
for high demanding automotive and industrial applications&lt;br&gt;
(e.g. engine management, starter generator, 3-phase motor control or robotics) &lt;br&gt;
Source: http://www.infineon.com ..</description>
<gates>
<gate name="PORT12" symbol="PORT16"/>
<gate name="PORT13" symbol="PORT16"/>
<gate name="P8/GPTA" symbol="PORT16"/>
<gate name="P9/GPTA" symbol="PORT16"/>
<gate name="PORT10" symbol="PORT16"/>
<gate name="PORT11" symbol="PORT16"/>
<gate name="P5/TRACE" symbol="PORT16"/>
<gate name="P6/ADC0" symbol="PORT16"/>
<gate name="P7/ADC1" symbol="PORT16"/>
<gate name="AD0-15" symbol="PORT16"/>
<gate name="AD16-31" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="P3" symbol="PORT16"/>
<gate name="P4" symbol="PORT16"/>
<gate name="NC" symbol="NC10"/>
<gate name="PWR1-2.5V" symbol="VSS_VDD"/>
<gate name="PWR2-2.5V" symbol="VSS_VDD"/>
<gate name="PWR3-2.5V" symbol="VSS_VDD"/>
<gate name="PWR4-2.5V" symbol="VSS_VDD"/>
<gate name="PWR5-2.5V" symbol="VSS_VDD"/>
<gate name="PWR6-3.3V" symbol="VSS_VDD"/>
<gate name="PWR7-3.3V" symbol="VSS_VDD"/>
<gate name="PWR8-3.3V" symbol="VSS_VDD"/>
<gate name="PWR9-3.3V" symbol="VSS_VDD"/>
<gate name="PWR10-3.3V" symbol="VSS_VDD"/>
<gate name="PWR11-3.3V" symbol="VSS_VDD"/>
<gate name="PWR12-2.5V" symbol="VSS_VDD"/>
<gate name="PWR13-2.5V" symbol="VSS_VDD"/>
<gate name="PWR14-2.5V" symbol="VSS_VDD"/>
<gate name="PWR15-2.5V" symbol="VSS_VDD"/>
<gate name="P-SB-2.5V" symbol="VSS_VDD"/>
<gate name="P-SRAM1-2.5V" symbol="VSS_VDD"/>
<gate name="P-SRAM2-2.5V" symbol="VSS_VDD"/>
<gate name="PWR16-2.5V" symbol="VSS_VDD"/>
<gate name="PWR17-2.5V" symbol="VSS_VDD"/>
<gate name="PWR18-2.5V" symbol="VSS_VDD"/>
<gate name="PWR19-2.5V" symbol="VSS_VDD"/>
<gate name="PWR20-2.5V" symbol="VSS_VDD"/>
<gate name="PWR21-2.5V" symbol="VSS_VDD"/>
<gate name="P-SC-5V" symbol="VSS_VDD"/>
<gate name="P-DM-5V" symbol="VSS_VDD"/>
<gate name="JTAG" symbol="JTAG-OCSD"/>
<gate name="A" symbol="TC1775"/>
<gate name="PWR22" symbol="VSS"/>
<gate name="PWR23" symbol="VSS"/>
<gate name="PWR24" symbol="VSS"/>
<gate name="PWR25" symbol="VSS"/>
<gate name="PWR26" symbol="VSS"/>
</gates>
<devices>
<device name="" package="P-BGA329">
<connects>
<connect gate="A" pin="BYPASS" pad="W22"/>
<connect gate="A" pin="CFG0" pad="Y23"/>
<connect gate="A" pin="CFG1" pad="Y22"/>
<connect gate="A" pin="CFG2" pad="W21"/>
<connect gate="A" pin="CFG3" pad="W23"/>
<connect gate="A" pin="CLKIN" pad="T1"/>
<connect gate="A" pin="CLKOUT" pad="R1"/>
<connect gate="A" pin="CLKSEL0" pad="V21"/>
<connect gate="A" pin="CLKSEL1" pad="V23"/>
<connect gate="A" pin="CLKSEL2" pad="V22"/>
<connect gate="A" pin="HDRST" pad="W20"/>
<connect gate="A" pin="NMI" pad="Y20"/>
<connect gate="A" pin="PORST" pad="Y21"/>
<connect gate="A" pin="TESTMODE" pad="AB23"/>
<connect gate="A" pin="VAGND@0" pad="B8"/>
<connect gate="A" pin="VAGND@1" pad="G4"/>
<connect gate="A" pin="VAREF@0" pad="C8"/>
<connect gate="A" pin="VAREF@1" pad="G2"/>
<connect gate="A" pin="VDD@0" pad="AC21"/>
<connect gate="A" pin="VDD@1" pad="AA22"/>
<connect gate="A" pin="VDDA@0" pad="D9"/>
<connect gate="A" pin="VDDA@1" pad="H1"/>
<connect gate="A" pin="VSS@0" pad="AA21"/>
<connect gate="A" pin="VSS@1" pad="AA23"/>
<connect gate="A" pin="VSSA@0" pad="A9"/>
<connect gate="A" pin="VSSA@1" pad="G3"/>
<connect gate="A" pin="XTAL1" pad="AC23"/>
<connect gate="A" pin="XTAL2" pad="AC22"/>
<connect gate="A" pin="XTAL3" pad="AB21"/>
<connect gate="A" pin="XTAL4" pad="AA20"/>
<connect gate="AD0-15" pin="0" pad="N1"/>
<connect gate="AD0-15" pin="1" pad="N4"/>
<connect gate="AD0-15" pin="10" pad="U3"/>
<connect gate="AD0-15" pin="11" pad="U2"/>
<connect gate="AD0-15" pin="12" pad="U4"/>
<connect gate="AD0-15" pin="13" pad="U1"/>
<connect gate="AD0-15" pin="14" pad="V2"/>
<connect gate="AD0-15" pin="15" pad="V1"/>
<connect gate="AD0-15" pin="2" pad="P3"/>
<connect gate="AD0-15" pin="3" pad="P2"/>
<connect gate="AD0-15" pin="4" pad="P1"/>
<connect gate="AD0-15" pin="5" pad="R3"/>
<connect gate="AD0-15" pin="6" pad="R2"/>
<connect gate="AD0-15" pin="7" pad="R4"/>
<connect gate="AD0-15" pin="8" pad="T3"/>
<connect gate="AD0-15" pin="9" pad="T2"/>
<connect gate="AD16-31" pin="0" pad="H2"/>
<connect gate="AD16-31" pin="1" pad="H3"/>
<connect gate="AD16-31" pin="10" pad="L3"/>
<connect gate="AD16-31" pin="11" pad="M3"/>
<connect gate="AD16-31" pin="12" pad="M1"/>
<connect gate="AD16-31" pin="13" pad="M2"/>
<connect gate="AD16-31" pin="14" pad="N2"/>
<connect gate="AD16-31" pin="15" pad="N3"/>
<connect gate="AD16-31" pin="2" pad="J1"/>
<connect gate="AD16-31" pin="3" pad="J4"/>
<connect gate="AD16-31" pin="4" pad="J2"/>
<connect gate="AD16-31" pin="5" pad="J3"/>
<connect gate="AD16-31" pin="6" pad="K1"/>
<connect gate="AD16-31" pin="7" pad="K2"/>
<connect gate="AD16-31" pin="8" pad="L1"/>
<connect gate="AD16-31" pin="9" pad="L2"/>
<connect gate="JTAG" pin="!BRKIN" pad="AC20"/>
<connect gate="JTAG" pin="!BRKOUT" pad="AC18"/>
<connect gate="JTAG" pin="!OCDSE" pad="Y19"/>
<connect gate="JTAG" pin="!TRST" pad="AA19"/>
<connect gate="JTAG" pin="TCK" pad="AB19"/>
<connect gate="JTAG" pin="TDI" pad="AC19"/>
<connect gate="JTAG" pin="TDO" pad="AA18"/>
<connect gate="JTAG" pin="TMS" pad="AB20"/>
<connect gate="NC" pin="NC@0" pad="AB15"/>
<connect gate="NC" pin="NC@1" pad="D10"/>
<connect gate="NC" pin="NC@2" pad="Y14"/>
<connect gate="NC" pin="NC@3" pad="AB22"/>
<connect gate="NC" pin="NC@4" pad="C14"/>
<connect gate="NC" pin="NC@5" pad="K3"/>
<connect gate="NC" pin="NC@6" pad="AC3"/>
<connect gate="NC" pin="NC@7" pad="L4"/>
<connect gate="NC" pin="NC@8" pad="D21"/>
<connect gate="NC" pin="NC@9" pad="Y16"/>
<connect gate="P-DM-5V" pin="VDD" pad="C3"/>
<connect gate="P-DM-5V" pin="VSS" pad="N12"/>
<connect gate="P-SB-2.5V" pin="VDD" pad="B14"/>
<connect gate="P-SB-2.5V" pin="VSS" pad="N13"/>
<connect gate="P-SC-5V" pin="VDD" pad="A1"/>
<connect gate="P-SC-5V" pin="VSS" pad="A2"/>
<connect gate="P-SRAM1-2.5V" pin="VDD" pad="AC17"/>
<connect gate="P-SRAM1-2.5V" pin="VSS" pad="N14"/>
<connect gate="P-SRAM2-2.5V" pin="VDD" pad="AB18"/>
<connect gate="P-SRAM2-2.5V" pin="VSS" pad="A3"/>
<connect gate="P2" pin="0" pad="AB3"/>
<connect gate="P2" pin="1" pad="AA4"/>
<connect gate="P2" pin="10" pad="AB6"/>
<connect gate="P2" pin="11" pad="AC7"/>
<connect gate="P2" pin="12" pad="Y7"/>
<connect gate="P2" pin="13" pad="AB7"/>
<connect gate="P2" pin="14" pad="AA7"/>
<connect gate="P2" pin="15" pad="AC8"/>
<connect gate="P2" pin="2" pad="Y5"/>
<connect gate="P2" pin="3" pad="AC4"/>
<connect gate="P2" pin="4" pad="AB4"/>
<connect gate="P2" pin="5" pad="AA5"/>
<connect gate="P2" pin="6" pad="AC5"/>
<connect gate="P2" pin="7" pad="AB5"/>
<connect gate="P2" pin="8" pad="AA6"/>
<connect gate="P2" pin="9" pad="AC6"/>
<connect gate="P3" pin="0" pad="AB8"/>
<connect gate="P3" pin="1" pad="AA8"/>
<connect gate="P3" pin="10" pad="AC11"/>
<connect gate="P3" pin="11" pad="AB11"/>
<connect gate="P3" pin="12" pad="AA11"/>
<connect gate="P3" pin="13" pad="AA12"/>
<connect gate="P3" pin="14" pad="AC12"/>
<connect gate="P3" pin="15" pad="AB12"/>
<connect gate="P3" pin="2" pad="AC9"/>
<connect gate="P3" pin="3" pad="Y9"/>
<connect gate="P3" pin="4" pad="AB9"/>
<connect gate="P3" pin="5" pad="AA9"/>
<connect gate="P3" pin="6" pad="AC10"/>
<connect gate="P3" pin="7" pad="AB10"/>
<connect gate="P3" pin="8" pad="AA10"/>
<connect gate="P3" pin="9" pad="Y11"/>
<connect gate="P4" pin="0" pad="V3"/>
<connect gate="P4" pin="1" pad="W2"/>
<connect gate="P4" pin="10" pad="AA3"/>
<connect gate="P4" pin="11" pad="AB1"/>
<connect gate="P4" pin="12" pad="AC1"/>
<connect gate="P4" pin="13" pad="AC2"/>
<connect gate="P4" pin="14" pad="AB2"/>
<connect gate="P4" pin="15" pad="Y4"/>
<connect gate="P4" pin="2" pad="W1"/>
<connect gate="P4" pin="3" pad="W3"/>
<connect gate="P4" pin="4" pad="Y2"/>
<connect gate="P4" pin="5" pad="Y1"/>
<connect gate="P4" pin="6" pad="W4"/>
<connect gate="P4" pin="7" pad="Y3"/>
<connect gate="P4" pin="8" pad="AA2"/>
<connect gate="P4" pin="9" pad="AA1"/>
<connect gate="P5/TRACE" pin="0" pad="AB13"/>
<connect gate="P5/TRACE" pin="1" pad="AA13"/>
<connect gate="P5/TRACE" pin="10" pad="AA16"/>
<connect gate="P5/TRACE" pin="11" pad="AB16"/>
<connect gate="P5/TRACE" pin="12" pad="AC16"/>
<connect gate="P5/TRACE" pin="13" pad="AA17"/>
<connect gate="P5/TRACE" pin="14" pad="AB17"/>
<connect gate="P5/TRACE" pin="15" pad="Y17"/>
<connect gate="P5/TRACE" pin="2" pad="AC13"/>
<connect gate="P5/TRACE" pin="3" pad="Y13"/>
<connect gate="P5/TRACE" pin="4" pad="AA14"/>
<connect gate="P5/TRACE" pin="5" pad="AB14"/>
<connect gate="P5/TRACE" pin="6" pad="AC14"/>
<connect gate="P5/TRACE" pin="7" pad="AA15"/>
<connect gate="P5/TRACE" pin="8" pad="Y15"/>
<connect gate="P5/TRACE" pin="9" pad="AC15"/>
<connect gate="P6/ADC0" pin="0" pad="B3"/>
<connect gate="P6/ADC0" pin="1" pad="C4"/>
<connect gate="P6/ADC0" pin="10" pad="B6"/>
<connect gate="P6/ADC0" pin="11" pad="A7"/>
<connect gate="P6/ADC0" pin="12" pad="D7"/>
<connect gate="P6/ADC0" pin="13" pad="B7"/>
<connect gate="P6/ADC0" pin="14" pad="C7"/>
<connect gate="P6/ADC0" pin="15" pad="A8"/>
<connect gate="P6/ADC0" pin="2" pad="D5"/>
<connect gate="P6/ADC0" pin="3" pad="A4"/>
<connect gate="P6/ADC0" pin="4" pad="B4"/>
<connect gate="P6/ADC0" pin="5" pad="C5"/>
<connect gate="P6/ADC0" pin="6" pad="A5"/>
<connect gate="P6/ADC0" pin="7" pad="B5"/>
<connect gate="P6/ADC0" pin="8" pad="C6"/>
<connect gate="P6/ADC0" pin="9" pad="A6"/>
<connect gate="P7/ADC1" pin="0" pad="B1"/>
<connect gate="P7/ADC1" pin="1" pad="B2"/>
<connect gate="P7/ADC1" pin="10" pad="E1"/>
<connect gate="P7/ADC1" pin="11" pad="E2"/>
<connect gate="P7/ADC1" pin="12" pad="F3"/>
<connect gate="P7/ADC1" pin="13" pad="F1"/>
<connect gate="P7/ADC1" pin="14" pad="F2"/>
<connect gate="P7/ADC1" pin="15" pad="G1"/>
<connect gate="P7/ADC1" pin="2" pad="D4"/>
<connect gate="P7/ADC1" pin="3" pad="C1"/>
<connect gate="P7/ADC1" pin="4" pad="C2"/>
<connect gate="P7/ADC1" pin="5" pad="D3"/>
<connect gate="P7/ADC1" pin="6" pad="E4"/>
<connect gate="P7/ADC1" pin="7" pad="D1"/>
<connect gate="P7/ADC1" pin="8" pad="D2"/>
<connect gate="P7/ADC1" pin="9" pad="E3"/>
<connect gate="P8/GPTA" pin="0" pad="U23"/>
<connect gate="P8/GPTA" pin="1" pad="U20"/>
<connect gate="P8/GPTA" pin="10" pad="R21"/>
<connect gate="P8/GPTA" pin="11" pad="P23"/>
<connect gate="P8/GPTA" pin="12" pad="P22"/>
<connect gate="P8/GPTA" pin="13" pad="P21"/>
<connect gate="P8/GPTA" pin="14" pad="N20"/>
<connect gate="P8/GPTA" pin="15" pad="N23"/>
<connect gate="P8/GPTA" pin="2" pad="U22"/>
<connect gate="P8/GPTA" pin="3" pad="U21"/>
<connect gate="P8/GPTA" pin="4" pad="T23"/>
<connect gate="P8/GPTA" pin="5" pad="T22"/>
<connect gate="P8/GPTA" pin="6" pad="T21"/>
<connect gate="P8/GPTA" pin="7" pad="R23"/>
<connect gate="P8/GPTA" pin="8" pad="R20"/>
<connect gate="P8/GPTA" pin="9" pad="R22"/>
<connect gate="P9/GPTA" pin="0" pad="N22"/>
<connect gate="P9/GPTA" pin="1" pad="N21"/>
<connect gate="P9/GPTA" pin="10" pad="K22"/>
<connect gate="P9/GPTA" pin="11" pad="K23"/>
<connect gate="P9/GPTA" pin="12" pad="J21"/>
<connect gate="P9/GPTA" pin="13" pad="J22"/>
<connect gate="P9/GPTA" pin="14" pad="J20"/>
<connect gate="P9/GPTA" pin="15" pad="J23"/>
<connect gate="P9/GPTA" pin="2" pad="M21"/>
<connect gate="P9/GPTA" pin="3" pad="M23"/>
<connect gate="P9/GPTA" pin="4" pad="M22"/>
<connect gate="P9/GPTA" pin="5" pad="L22"/>
<connect gate="P9/GPTA" pin="6" pad="L21"/>
<connect gate="P9/GPTA" pin="7" pad="L23"/>
<connect gate="P9/GPTA" pin="8" pad="L20"/>
<connect gate="P9/GPTA" pin="9" pad="K21"/>
<connect gate="PORT10" pin="0" pad="H21"/>
<connect gate="PORT10" pin="1" pad="H22"/>
<connect gate="PORT10" pin="10" pad="E22"/>
<connect gate="PORT10" pin="11" pad="E23"/>
<connect gate="PORT10" pin="12" pad="E21"/>
<connect gate="PORT10" pin="13" pad="D22"/>
<connect gate="PORT10" pin="14" pad="D23"/>
<connect gate="PORT10" pin="15" pad="E20"/>
<connect gate="PORT10" pin="2" pad="H23"/>
<connect gate="PORT10" pin="3" pad="G21"/>
<connect gate="PORT10" pin="4" pad="G22"/>
<connect gate="PORT10" pin="5" pad="G20"/>
<connect gate="PORT10" pin="6" pad="G23"/>
<connect gate="PORT10" pin="7" pad="F22"/>
<connect gate="PORT10" pin="8" pad="F23"/>
<connect gate="PORT10" pin="9" pad="F21"/>
<connect gate="PORT11" pin="0" pad="C22"/>
<connect gate="PORT11" pin="1" pad="C23"/>
<connect gate="PORT11" pin="10" pad="C20"/>
<connect gate="PORT11" pin="11" pad="D19"/>
<connect gate="PORT11" pin="12" pad="A20"/>
<connect gate="PORT11" pin="13" pad="B20"/>
<connect gate="PORT11" pin="14" pad="C19"/>
<connect gate="PORT11" pin="15" pad="A19"/>
<connect gate="PORT11" pin="2" pad="C21"/>
<connect gate="PORT11" pin="3" pad="B23"/>
<connect gate="PORT11" pin="4" pad="A23"/>
<connect gate="PORT11" pin="5" pad="A22"/>
<connect gate="PORT11" pin="6" pad="B22"/>
<connect gate="PORT11" pin="7" pad="D20"/>
<connect gate="PORT11" pin="8" pad="A21"/>
<connect gate="PORT11" pin="9" pad="B21"/>
<connect gate="PORT12" pin="0" pad="D13"/>
<connect gate="PORT12" pin="1" pad="A13"/>
<connect gate="PORT12" pin="10" pad="D11"/>
<connect gate="PORT12" pin="11" pad="C10"/>
<connect gate="PORT12" pin="12" pad="B10"/>
<connect gate="PORT12" pin="13" pad="A10"/>
<connect gate="PORT12" pin="14" pad="C9"/>
<connect gate="PORT12" pin="15" pad="B9"/>
<connect gate="PORT12" pin="2" pad="B13"/>
<connect gate="PORT12" pin="3" pad="C13"/>
<connect gate="PORT12" pin="4" pad="C12"/>
<connect gate="PORT12" pin="5" pad="A12"/>
<connect gate="PORT12" pin="6" pad="B12"/>
<connect gate="PORT12" pin="7" pad="B11"/>
<connect gate="PORT12" pin="8" pad="C11"/>
<connect gate="PORT12" pin="9" pad="A11"/>
<connect gate="PORT13" pin="0" pad="B19"/>
<connect gate="PORT13" pin="1" pad="C18"/>
<connect gate="PORT13" pin="10" pad="C16"/>
<connect gate="PORT13" pin="11" pad="A15"/>
<connect gate="PORT13" pin="12" pad="D15"/>
<connect gate="PORT13" pin="13" pad="B15"/>
<connect gate="PORT13" pin="14" pad="C15"/>
<connect gate="PORT13" pin="15" pad="A14"/>
<connect gate="PORT13" pin="2" pad="A18"/>
<connect gate="PORT13" pin="3" pad="B18"/>
<connect gate="PORT13" pin="4" pad="A17"/>
<connect gate="PORT13" pin="5" pad="D17"/>
<connect gate="PORT13" pin="6" pad="B17"/>
<connect gate="PORT13" pin="7" pad="C17"/>
<connect gate="PORT13" pin="8" pad="A16"/>
<connect gate="PORT13" pin="9" pad="B16"/>
<connect gate="PWR1-2.5V" pin="VDD" pad="H4"/>
<connect gate="PWR1-2.5V" pin="VSS" pad="F4"/>
<connect gate="PWR10-3.3V" pin="VDD" pad="M20"/>
<connect gate="PWR10-3.3V" pin="VSS" pad="L10"/>
<connect gate="PWR11-3.3V" pin="VDD" pad="T20"/>
<connect gate="PWR11-3.3V" pin="VSS" pad="L11"/>
<connect gate="PWR12-2.5V" pin="VDD" pad="K4"/>
<connect gate="PWR12-2.5V" pin="VSS" pad="L12"/>
<connect gate="PWR13-2.5V" pin="VDD" pad="P4"/>
<connect gate="PWR13-2.5V" pin="VSS" pad="L13"/>
<connect gate="PWR14-2.5V" pin="VDD" pad="V4"/>
<connect gate="PWR14-2.5V" pin="VSS" pad="L14"/>
<connect gate="PWR15-2.5V" pin="VDD" pad="D6"/>
<connect gate="PWR15-2.5V" pin="VSS" pad="P10"/>
<connect gate="PWR16-2.5V" pin="VDD" pad="D14"/>
<connect gate="PWR16-2.5V" pin="VSS" pad="M10"/>
<connect gate="PWR17-2.5V" pin="VDD" pad="Y10"/>
<connect gate="PWR17-2.5V" pin="VSS" pad="M11"/>
<connect gate="PWR18-2.5V" pin="VDD" pad="Y18"/>
<connect gate="PWR18-2.5V" pin="VSS" pad="M12"/>
<connect gate="PWR19-2.5V" pin="VDD" pad="F20"/>
<connect gate="PWR19-2.5V" pin="VSS" pad="M13"/>
<connect gate="PWR2-2.5V" pin="VDD" pad="M4"/>
<connect gate="PWR2-2.5V" pin="VSS" pad="Y6"/>
<connect gate="PWR20-2.5V" pin="VDD" pad="K20"/>
<connect gate="PWR20-2.5V" pin="VSS" pad="M14"/>
<connect gate="PWR21-2.5V" pin="VDD" pad="P20"/>
<connect gate="PWR21-2.5V" pin="VSS" pad="P13"/>
<connect gate="PWR22" pin="VSS" pad="P11"/>
<connect gate="PWR23" pin="VSS" pad="P12"/>
<connect gate="PWR24" pin="VSS" pad="P14"/>
<connect gate="PWR25" pin="VSS" pad="N10"/>
<connect gate="PWR26" pin="VSS" pad="N11"/>
<connect gate="PWR3-2.5V" pin="VDD" pad="T4"/>
<connect gate="PWR3-2.5V" pin="VSS" pad="V20"/>
<connect gate="PWR4-2.5V" pin="VDD" pad="Y8"/>
<connect gate="PWR4-2.5V" pin="VSS" pad="D18"/>
<connect gate="PWR5-2.5V" pin="VDD" pad="Y12"/>
<connect gate="PWR5-2.5V" pin="VSS" pad="K10"/>
<connect gate="PWR6-3.3V" pin="VDD" pad="D8"/>
<connect gate="PWR6-3.3V" pin="VSS" pad="K11"/>
<connect gate="PWR7-3.3V" pin="VDD" pad="D12"/>
<connect gate="PWR7-3.3V" pin="VSS" pad="K12"/>
<connect gate="PWR8-3.3V" pin="VDD" pad="D16"/>
<connect gate="PWR8-3.3V" pin="VSS" pad="K13"/>
<connect gate="PWR9-3.3V" pin="VDD" pad="H20"/>
<connect gate="PWR9-3.3V" pin="VSS" pad="K14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1920" prefix="IC">
<description>&lt;b&gt;32bit Single Chip Microcontroller&lt;/b&gt;&lt;p&gt;
Source: http://www.infineon.com .. TC1920_umsu_V12.pdf</description>
<gates>
<gate name="DEBUG" symbol="JTAG-OCSD"/>
<gate name="P3" symbol="PORT16"/>
<gate name="P2" symbol="PORT16"/>
<gate name="AD" symbol="D31"/>
<gate name="P1" symbol="PORT8"/>
<gate name="P0" symbol="PORT8"/>
<gate name="EBU" symbol="A23"/>
<gate name="P5/TRACE" symbol="PORT16"/>
<gate name="PWR" symbol="TC1920PWR"/>
<gate name="PWR2" symbol="TC1920PWR2"/>
<gate name="G" symbol="TC1920"/>
</gates>
<devices>
<device name="" package="P-LBGA-260">
<connects>
<connect gate="AD" pin="D0" pad="L3"/>
<connect gate="AD" pin="D1" pad="L2"/>
<connect gate="AD" pin="D10" pad="H1"/>
<connect gate="AD" pin="D11" pad="H2"/>
<connect gate="AD" pin="D12" pad="H3"/>
<connect gate="AD" pin="D13" pad="G1"/>
<connect gate="AD" pin="D14" pad="G2"/>
<connect gate="AD" pin="D15" pad="G3"/>
<connect gate="AD" pin="D16" pad="H4"/>
<connect gate="AD" pin="D17" pad="G4"/>
<connect gate="AD" pin="D18" pad="E4"/>
<connect gate="AD" pin="D19" pad="F1"/>
<connect gate="AD" pin="D2" pad="K3"/>
<connect gate="AD" pin="D20" pad="F2"/>
<connect gate="AD" pin="D21" pad="F4"/>
<connect gate="AD" pin="D22" pad="F3"/>
<connect gate="AD" pin="D23" pad="E1"/>
<connect gate="AD" pin="D24" pad="E2"/>
<connect gate="AD" pin="D25" pad="E3"/>
<connect gate="AD" pin="D26" pad="D1"/>
<connect gate="AD" pin="D27" pad="C1"/>
<connect gate="AD" pin="D28" pad="D2"/>
<connect gate="AD" pin="D29" pad="D3"/>
<connect gate="AD" pin="D3" pad="K4"/>
<connect gate="AD" pin="D30" pad="C2"/>
<connect gate="AD" pin="D31" pad="B1"/>
<connect gate="AD" pin="D4" pad="L1"/>
<connect gate="AD" pin="D5" pad="K2"/>
<connect gate="AD" pin="D6" pad="K1"/>
<connect gate="AD" pin="D7" pad="J3"/>
<connect gate="AD" pin="D8" pad="J1"/>
<connect gate="AD" pin="D9" pad="J2"/>
<connect gate="DEBUG" pin="!BRKIN" pad="U15"/>
<connect gate="DEBUG" pin="!BRKOUT" pad="T14"/>
<connect gate="DEBUG" pin="!OCDSE" pad="V16"/>
<connect gate="DEBUG" pin="!TRST" pad="U17"/>
<connect gate="DEBUG" pin="TCK" pad="T16"/>
<connect gate="DEBUG" pin="TDI" pad="V17"/>
<connect gate="DEBUG" pin="TDO" pad="U16"/>
<connect gate="DEBUG" pin="TMS" pad="T15"/>
<connect gate="EBU" pin="A0" pad="V2"/>
<connect gate="EBU" pin="A1" pad="T5"/>
<connect gate="EBU" pin="A10" pad="T1"/>
<connect gate="EBU" pin="A11" pad="P3"/>
<connect gate="EBU" pin="A12" pad="R5"/>
<connect gate="EBU" pin="A13" pad="R2"/>
<connect gate="EBU" pin="A14" pad="P2"/>
<connect gate="EBU" pin="A15" pad="N3"/>
<connect gate="EBU" pin="A16" pad="R1"/>
<connect gate="EBU" pin="A17" pad="P1"/>
<connect gate="EBU" pin="A18" pad="N2"/>
<connect gate="EBU" pin="A19" pad="P4"/>
<connect gate="EBU" pin="A2" pad="V1"/>
<connect gate="EBU" pin="A20" pad="M3"/>
<connect gate="EBU" pin="A21" pad="N4"/>
<connect gate="EBU" pin="A22" pad="M4"/>
<connect gate="EBU" pin="A23" pad="N1"/>
<connect gate="EBU" pin="A3" pad="U3"/>
<connect gate="EBU" pin="A4" pad="T4"/>
<connect gate="EBU" pin="A5" pad="U2"/>
<connect gate="EBU" pin="A6" pad="T3"/>
<connect gate="EBU" pin="A7" pad="U1"/>
<connect gate="EBU" pin="A8" pad="R3"/>
<connect gate="EBU" pin="A9" pad="T2"/>
<connect gate="G" pin="/ADV" pad="R10"/>
<connect gate="G" pin="/BAA" pad="U8"/>
<connect gate="G" pin="/BC0" pad="T7"/>
<connect gate="G" pin="/BC1" pad="R6"/>
<connect gate="G" pin="/BC2" pad="V4"/>
<connect gate="G" pin="/BC3" pad="U6"/>
<connect gate="G" pin="/CAS" pad="T6"/>
<connect gate="G" pin="/CMDELAY" pad="V9"/>
<connect gate="G" pin="/CSGLB" pad="U9"/>
<connect gate="G" pin="/RAS" pad="U5"/>
<connect gate="G" pin="/RD" pad="U4"/>
<connect gate="G" pin="/SCAN_MODE" pad="K15"/>
<connect gate="G" pin="/WAIT" pad="T8"/>
<connect gate="G" pin="/WR" pad="V3"/>
<connect gate="G" pin="AI0+" pad="D13"/>
<connect gate="G" pin="AI0-" pad="A13"/>
<connect gate="G" pin="AI1+" pad="D14"/>
<connect gate="G" pin="AI1-" pad="A14"/>
<connect gate="G" pin="ALE" pad="T10"/>
<connect gate="G" pin="AO0+" pad="A15"/>
<connect gate="G" pin="AO0-" pad="B15"/>
<connect gate="G" pin="AO1+" pad="C14"/>
<connect gate="G" pin="AO1-" pad="B14"/>
<connect gate="G" pin="BFCLK0" pad="M2"/>
<connect gate="G" pin="BYPASS" pad="B17"/>
<connect gate="G" pin="CEXT" pad="A17"/>
<connect gate="G" pin="CKE" pad="U10"/>
<connect gate="G" pin="CLKOUT" pad="C17"/>
<connect gate="G" pin="CODEC_DIS" pad="C16"/>
<connect gate="G" pin="CS0" pad="R9"/>
<connect gate="G" pin="CS1" pad="R8"/>
<connect gate="G" pin="CS2" pad="R7"/>
<connect gate="G" pin="CS3" pad="V7"/>
<connect gate="G" pin="CS4" pad="V6"/>
<connect gate="G" pin="CS5" pad="V5"/>
<connect gate="G" pin="CS6" pad="U7"/>
<connect gate="G" pin="CSEMU" pad="V8"/>
<connect gate="G" pin="CSOVL" pad="T9"/>
<connect gate="G" pin="EBUCLK" pad="M1"/>
<connect gate="G" pin="HRST" pad="D16"/>
<connect gate="G" pin="MR/W" pad="V10"/>
<connect gate="G" pin="NMI" pad="A18"/>
<connect gate="G" pin="P4.0/AIN0" pad="C11"/>
<connect gate="G" pin="P4.1/AIN1" pad="A11"/>
<connect gate="G" pin="P4.2/AIN2" pad="B10"/>
<connect gate="G" pin="P4.3/AIN3" pad="A10"/>
<connect gate="G" pin="P4.4/AIN4" pad="C10"/>
<connect gate="G" pin="P4.5/AIN5" pad="A9"/>
<connect gate="G" pin="PLLCTRL_A0" pad="B8"/>
<connect gate="G" pin="PORST" pad="B18"/>
<connect gate="G" pin="TM_CTRL0" pad="B4"/>
<connect gate="G" pin="TM_CTRL1" pad="A3"/>
<connect gate="G" pin="VDDP_OSC" pad="D7"/>
<connect gate="G" pin="VDD_OSC1" pad="A7"/>
<connect gate="G" pin="VDD_OSC2" pad="C6"/>
<connect gate="G" pin="VSS_OSC" pad="B6"/>
<connect gate="G" pin="XTAL1" pad="A6"/>
<connect gate="G" pin="XTAL2" pad="B7"/>
<connect gate="G" pin="XTAL3" pad="A4"/>
<connect gate="G" pin="XTAL4" pad="B5"/>
<connect gate="P0" pin="0" pad="R18"/>
<connect gate="P0" pin="1" pad="N16"/>
<connect gate="P0" pin="2" pad="N17"/>
<connect gate="P0" pin="3" pad="P15"/>
<connect gate="P0" pin="4" pad="P18"/>
<connect gate="P0" pin="5" pad="N18"/>
<connect gate="P0" pin="6" pad="N15"/>
<connect gate="P0" pin="7" pad="M15"/>
<connect gate="P1" pin="0" pad="V18"/>
<connect gate="P1" pin="1" pad="R16"/>
<connect gate="P1" pin="2" pad="P16"/>
<connect gate="P1" pin="3" pad="T17"/>
<connect gate="P1" pin="4" pad="U18"/>
<connect gate="P1" pin="5" pad="R17"/>
<connect gate="P1" pin="6" pad="T18"/>
<connect gate="P1" pin="7" pad="P17"/>
<connect gate="P2" pin="0" pad="G18"/>
<connect gate="P2" pin="1" pad="G17"/>
<connect gate="P2" pin="10" pad="D18"/>
<connect gate="P2" pin="11" pad="C18"/>
<connect gate="P2" pin="12" pad="F16"/>
<connect gate="P2" pin="13" pad="D17"/>
<connect gate="P2" pin="14" pad="E16"/>
<connect gate="P2" pin="15" pad="F15"/>
<connect gate="P2" pin="2" pad="H16"/>
<connect gate="P2" pin="3" pad="F18"/>
<connect gate="P2" pin="4" pad="E18"/>
<connect gate="P2" pin="5" pad="F17"/>
<connect gate="P2" pin="6" pad="H15"/>
<connect gate="P2" pin="7" pad="G16"/>
<connect gate="P2" pin="8" pad="E17"/>
<connect gate="P2" pin="9" pad="G15"/>
<connect gate="P3" pin="0" pad="L15"/>
<connect gate="P3" pin="1" pad="M16"/>
<connect gate="P3" pin="10" pad="K16"/>
<connect gate="P3" pin="11" pad="J17"/>
<connect gate="P3" pin="12" pad="J15"/>
<connect gate="P3" pin="13" pad="H18"/>
<connect gate="P3" pin="14" pad="H17"/>
<connect gate="P3" pin="15" pad="J16"/>
<connect gate="P3" pin="2" pad="M17"/>
<connect gate="P3" pin="3" pad="M18"/>
<connect gate="P3" pin="4" pad="L17"/>
<connect gate="P3" pin="5" pad="L16"/>
<connect gate="P3" pin="6" pad="L18"/>
<connect gate="P3" pin="7" pad="K17"/>
<connect gate="P3" pin="8" pad="K18"/>
<connect gate="P3" pin="9" pad="J18"/>
<connect gate="P5/TRACE" pin="0" pad="V15"/>
<connect gate="P5/TRACE" pin="1" pad="U14"/>
<connect gate="P5/TRACE" pin="10" pad="V13"/>
<connect gate="P5/TRACE" pin="11" pad="U12"/>
<connect gate="P5/TRACE" pin="12" pad="T11"/>
<connect gate="P5/TRACE" pin="13" pad="V12"/>
<connect gate="P5/TRACE" pin="14" pad="U11"/>
<connect gate="P5/TRACE" pin="15" pad="V11"/>
<connect gate="P5/TRACE" pin="2" pad="T13"/>
<connect gate="P5/TRACE" pin="3" pad="R14"/>
<connect gate="P5/TRACE" pin="4" pad="V14"/>
<connect gate="P5/TRACE" pin="5" pad="R13"/>
<connect gate="P5/TRACE" pin="6" pad="U13"/>
<connect gate="P5/TRACE" pin="7" pad="T12"/>
<connect gate="P5/TRACE" pin="8" pad="R12"/>
<connect gate="P5/TRACE" pin="9" pad="R11"/>
<connect gate="PWR" pin="1V8@0" pad="A16"/>
<connect gate="PWR" pin="1V8@1" pad="B16"/>
<connect gate="PWR" pin="1V8@2" pad="B3"/>
<connect gate="PWR" pin="1V8@3" pad="C4"/>
<connect gate="PWR" pin="1V8@4" pad="D5"/>
<connect gate="PWR" pin="1V8@5" pad="J4"/>
<connect gate="PWR" pin="1V8@6" pad="L4"/>
<connect gate="PWR" pin="1V8@7" pad="R4"/>
<connect gate="PWR" pin="3V3@0" pad="G11"/>
<connect gate="PWR" pin="3V3@1" pad="G12"/>
<connect gate="PWR" pin="3V3@10" pad="M7"/>
<connect gate="PWR" pin="3V3@11" pad="M8"/>
<connect gate="PWR" pin="3V3@2" pad="G7"/>
<connect gate="PWR" pin="3V3@3" pad="G8"/>
<connect gate="PWR" pin="3V3@4" pad="H12"/>
<connect gate="PWR" pin="3V3@5" pad="H7"/>
<connect gate="PWR" pin="3V3@6" pad="L12"/>
<connect gate="PWR" pin="3V3@7" pad="L7"/>
<connect gate="PWR" pin="3V3@8" pad="M11"/>
<connect gate="PWR" pin="3V3@9" pad="M12"/>
<connect gate="PWR" pin="GND@0" pad="A1"/>
<connect gate="PWR" pin="GND@1" pad="B2"/>
<connect gate="PWR" pin="GND@10" pad="H9"/>
<connect gate="PWR" pin="GND@11" pad="J10"/>
<connect gate="PWR" pin="GND@12" pad="J11"/>
<connect gate="PWR" pin="GND@13" pad="J12"/>
<connect gate="PWR" pin="GND@14" pad="J7"/>
<connect gate="PWR" pin="GND@15" pad="J8"/>
<connect gate="PWR" pin="GND@16" pad="J9"/>
<connect gate="PWR" pin="GND@17" pad="K10"/>
<connect gate="PWR" pin="GND@18" pad="K11"/>
<connect gate="PWR" pin="GND@19" pad="K12"/>
<connect gate="PWR" pin="GND@2" pad="C3"/>
<connect gate="PWR" pin="GND@20" pad="K7"/>
<connect gate="PWR" pin="GND@21" pad="K8"/>
<connect gate="PWR" pin="GND@22" pad="K9"/>
<connect gate="PWR" pin="GND@23" pad="L10"/>
<connect gate="PWR" pin="GND@24" pad="L11"/>
<connect gate="PWR" pin="GND@25" pad="L8"/>
<connect gate="PWR" pin="GND@26" pad="L9"/>
<connect gate="PWR" pin="GND@27" pad="M10"/>
<connect gate="PWR" pin="GND@28" pad="M9"/>
<connect gate="PWR" pin="GND@3" pad="D4"/>
<connect gate="PWR" pin="GND@4" pad="D6"/>
<connect gate="PWR" pin="GND@5" pad="G10"/>
<connect gate="PWR" pin="GND@6" pad="G9"/>
<connect gate="PWR" pin="GND@7" pad="H10"/>
<connect gate="PWR" pin="GND@8" pad="H11"/>
<connect gate="PWR" pin="GND@9" pad="H8"/>
<connect gate="PWR2" pin="VAGND_ADC" pad="B11"/>
<connect gate="PWR2" pin="VAREF_ADC" pad="D11"/>
<connect gate="PWR2" pin="VDDP_ADC" pad="C12"/>
<connect gate="PWR2" pin="VDDP_COD@0" pad="E15"/>
<connect gate="PWR2" pin="VDDP_OSC@1" pad="C7"/>
<connect gate="PWR2" pin="VDDR@0" pad="A2"/>
<connect gate="PWR2" pin="VDDR@1" pad="C5"/>
<connect gate="PWR2" pin="VDD_GUARD" pad="C9"/>
<connect gate="PWR2" pin="VDD_PLL" pad="D9"/>
<connect gate="PWR2" pin="VDD_SB" pad="R15"/>
<connect gate="PWR2" pin="VGND_COD" pad="C13"/>
<connect gate="PWR2" pin="VREF_COD" pad="B13"/>
<connect gate="PWR2" pin="VSSA_ADC" pad="A12"/>
<connect gate="PWR2" pin="VSSA_COD@0" pad="D15"/>
<connect gate="PWR2" pin="VSSP_ADC@0" pad="B12"/>
<connect gate="PWR2" pin="VSSP_ADC@1" pad="D12"/>
<connect gate="PWR2" pin="VSSP_ADC@2" pad="D10"/>
<connect gate="PWR2" pin="VSSP_COD@0" pad="C15"/>
<connect gate="PWR2" pin="VSSP_OSC@0" pad="D8"/>
<connect gate="PWR2" pin="VSSP_OSC@1" pad="A5"/>
<connect gate="PWR2" pin="VSS_GUARD@1" pad="A8"/>
<connect gate="PWR2" pin="VSS_GUARD@2" pad="C8"/>
<connect gate="PWR2" pin="VSS_PLL" pad="B9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TDA6060*" prefix="IC">
<description>&lt;b&gt;Phase locked loop&lt;/b&gt; (PLL)&lt;p&gt;
with a multistandard video modulator and a programmable sound FM and AM modulator</description>
<gates>
<gate name="G$1" symbol="TDA6060"/>
</gates>
<devices>
<device name="" package="P-TSSOP28-1">
<connects>
<connect gate="G$1" pin="AUDGND" pad="1"/>
<connect gate="G$1" pin="AUDINAM" pad="3"/>
<connect gate="G$1" pin="AUDINFM" pad="2"/>
<connect gate="G$1" pin="CAS" pad="5"/>
<connect gate="G$1" pin="CHGPMP" pad="16"/>
<connect gate="G$1" pin="GNDA" pad="23"/>
<connect gate="G$1" pin="GNDD" pad="9"/>
<connect gate="G$1" pin="MODGND" pad="7"/>
<connect gate="G$1" pin="MODOUT1" pad="6"/>
<connect gate="G$1" pin="MODOUT2" pad="8"/>
<connect gate="G$1" pin="O-B1" pad="19"/>
<connect gate="G$1" pin="O-B2" pad="22"/>
<connect gate="G$1" pin="O-C1" pad="21"/>
<connect gate="G$1" pin="O-C2" pad="20"/>
<connect gate="G$1" pin="P2/ADC" pad="15"/>
<connect gate="G$1" pin="Q" pad="13"/>
<connect gate="G$1" pin="QX" pad="14"/>
<connect gate="G$1" pin="SC2IN" pad="4"/>
<connect gate="G$1" pin="SCL" pad="11"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="SLF" pad="25"/>
<connect gate="G$1" pin="T1" pad="18"/>
<connect gate="G$1" pin="T2" pad="27"/>
<connect gate="G$1" pin="TFLF" pad="26"/>
<connect gate="G$1" pin="VCCA" pad="28"/>
<connect gate="G$1" pin="VCCD" pad="12"/>
<connect gate="G$1" pin="VIDIN" pad="24"/>
<connect gate="G$1" pin="VTUNE" pad="17"/>
</connects>
<technologies>
<technology name="G">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="XS">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLE6361G" prefix="IC">
<description>&lt;b&gt;Multi Voltage Microprocessor Power Supply&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TLE6361G"/>
</gates>
<devices>
<device name="" package="DSO36">
<connects>
<connect gate="G$1" pin="/CS" pad="3"/>
<connect gate="G$1" pin="/ERR" pad="6"/>
<connect gate="G$1" pin="BOOST" pad="33"/>
<connect gate="G$1" pin="BOOTSTRAP" pad="28"/>
<connect gate="G$1" pin="C+" pad="21"/>
<connect gate="G$1" pin="C-" pad="20"/>
<connect gate="G$1" pin="CCP" pad="22"/>
<connect gate="G$1" pin="CLK" pad="2"/>
<connect gate="G$1" pin="DI" pad="4"/>
<connect gate="G$1" pin="DO" pad="5"/>
<connect gate="G$1" pin="FB/L_IN@0" pad="25"/>
<connect gate="G$1" pin="FB/L_IN@1" pad="26"/>
<connect gate="G$1" pin="GND@0" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="18"/>
<connect gate="G$1" pin="GND@2" pad="19"/>
<connect gate="G$1" pin="GND@3" pad="36"/>
<connect gate="G$1" pin="IN@0" pad="30"/>
<connect gate="G$1" pin="IN@1" pad="32"/>
<connect gate="G$1" pin="Q_LDO1" pad="27"/>
<connect gate="G$1" pin="Q_LDO2" pad="24"/>
<connect gate="G$1" pin="Q_LDO3" pad="14"/>
<connect gate="G$1" pin="Q_STB" pad="7"/>
<connect gate="G$1" pin="Q_T1" pad="8"/>
<connect gate="G$1" pin="Q_T2" pad="9"/>
<connect gate="G$1" pin="Q_T3" pad="10"/>
<connect gate="G$1" pin="Q_T4" pad="11"/>
<connect gate="G$1" pin="Q_T5" pad="12"/>
<connect gate="G$1" pin="Q_T6" pad="13"/>
<connect gate="G$1" pin="R1" pad="17"/>
<connect gate="G$1" pin="R2" pad="16"/>
<connect gate="G$1" pin="R3" pad="15"/>
<connect gate="G$1" pin="SEL" pad="23"/>
<connect gate="G$1" pin="SLEW" pad="35"/>
<connect gate="G$1" pin="SWQ0" pad="29"/>
<connect gate="G$1" pin="SWQ1" pad="31"/>
<connect gate="G$1" pin="WAKE" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XC167" prefix="IC">
<description>&lt;b&gt;16-Bit Single-Chip Microcontrol ler&lt;/b&gt;&lt;p&gt;
Source: xc167_ds_v1.1_2003_06.pdf</description>
<gates>
<gate name="-POWER" symbol="XC167-POWER"/>
<gate name="-BUS-INTERFACE" symbol="XC167-BUS"/>
<gate name="-CLOCK-JTAG-OCDSI" symbol="XC167-CLOCK-JTAG"/>
<gate name="-PORTS" symbol="XC167-PORTS"/>
</gates>
<devices>
<device name="P" package="P-TQFP-144-19">
<connects>
<connect gate="-BUS-INTERFACE" pin="/NMI" pad="4"/>
<connect gate="-BUS-INTERFACE" pin="/RSTIN" pad="142"/>
<connect gate="-BUS-INTERFACE" pin="P0H.0-AD8" pad="105"/>
<connect gate="-BUS-INTERFACE" pin="P0H.1-AD9" pad="106"/>
<connect gate="-BUS-INTERFACE" pin="P0H.2-AD10" pad="111"/>
<connect gate="-BUS-INTERFACE" pin="P0H.3-AD11" pad="112"/>
<connect gate="-BUS-INTERFACE" pin="P0H.4-AD12" pad="113"/>
<connect gate="-BUS-INTERFACE" pin="P0H.5-AD13" pad="114"/>
<connect gate="-BUS-INTERFACE" pin="P0H.6-AD14" pad="115"/>
<connect gate="-BUS-INTERFACE" pin="P0H.7-AD15" pad="116"/>
<connect gate="-BUS-INTERFACE" pin="P0L.0-AD0" pad="95"/>
<connect gate="-BUS-INTERFACE" pin="P0L.1-AD1" pad="96"/>
<connect gate="-BUS-INTERFACE" pin="P0L.2-AD2" pad="97"/>
<connect gate="-BUS-INTERFACE" pin="P0L.3-AD3" pad="98"/>
<connect gate="-BUS-INTERFACE" pin="P0L.4-AD4" pad="99"/>
<connect gate="-BUS-INTERFACE" pin="P0L.5-AD5" pad="100"/>
<connect gate="-BUS-INTERFACE" pin="P0L.6-AD6" pad="101"/>
<connect gate="-BUS-INTERFACE" pin="P0L.7-AD7" pad="102"/>
<connect gate="-BUS-INTERFACE" pin="P1H.0-A8-/C6P0-CC23-E*" pad="127"/>
<connect gate="-BUS-INTERFACE" pin="P1H.1-A9-/C6P1-MRST1" pad="128"/>
<connect gate="-BUS-INTERFACE" pin="P1H.2-A10-/C6P2-MTSR1" pad="129"/>
<connect gate="-BUS-INTERFACE" pin="P1H.3-A11-SCLK1-E*" pad="130"/>
<connect gate="-BUS-INTERFACE" pin="P1H.4-A12-CC24IO" pad="131"/>
<connect gate="-BUS-INTERFACE" pin="P1H.5-A13-CC25IO" pad="132"/>
<connect gate="-BUS-INTERFACE" pin="P1H.6-A14-CC26IO" pad="133"/>
<connect gate="-BUS-INTERFACE" pin="P1H.7-A15-CC27IO" pad="134"/>
<connect gate="-BUS-INTERFACE" pin="P1L.0-A0-CC60" pad="117"/>
<connect gate="-BUS-INTERFACE" pin="P1L.1-A1-COUT60" pad="118"/>
<connect gate="-BUS-INTERFACE" pin="P1L.2-A2-CC61" pad="119"/>
<connect gate="-BUS-INTERFACE" pin="P1L.3-A3-COUT61" pad="120"/>
<connect gate="-BUS-INTERFACE" pin="P1L.4-A4-CC62" pad="121"/>
<connect gate="-BUS-INTERFACE" pin="P1L.5-A5-COUT62" pad="122"/>
<connect gate="-BUS-INTERFACE" pin="P1L.6-A6-COUT63" pad="123"/>
<connect gate="-BUS-INTERFACE" pin="P1L.7-A7-/CTRAP-CC22" pad="124"/>
<connect gate="-BUS-INTERFACE" pin="P20.0-/RD" pad="90"/>
<connect gate="-BUS-INTERFACE" pin="P20.1-/WR-/WRL" pad="91"/>
<connect gate="-BUS-INTERFACE" pin="P20.12-/RSTOUT" pad="3"/>
<connect gate="-BUS-INTERFACE" pin="P20.2-READY" pad="92"/>
<connect gate="-BUS-INTERFACE" pin="P20.4-ALE" pad="93"/>
<connect gate="-BUS-INTERFACE" pin="P20.5-/EA" pad="94"/>
<connect gate="-BUS-INTERFACE" pin="P3.12-/BHE-/WRH" pad="75"/>
<connect gate="-BUS-INTERFACE" pin="P4.0-A16" pad="80"/>
<connect gate="-BUS-INTERFACE" pin="P4.1-A17" pad="81"/>
<connect gate="-BUS-INTERFACE" pin="P4.2-A18" pad="82"/>
<connect gate="-BUS-INTERFACE" pin="P4.3-A19" pad="83"/>
<connect gate="-BUS-INTERFACE" pin="P4.4-A20-C*" pad="84"/>
<connect gate="-BUS-INTERFACE" pin="P4.5-A21-C*" pad="85"/>
<connect gate="-BUS-INTERFACE" pin="P4.6-A22-C*" pad="86"/>
<connect gate="-BUS-INTERFACE" pin="P4.7-A23-C*" pad="87"/>
<connect gate="-BUS-INTERFACE" pin="P6.0-/CS0-CC0IO" pad="7"/>
<connect gate="-BUS-INTERFACE" pin="P6.1-/CS1-CC1IO" pad="8"/>
<connect gate="-BUS-INTERFACE" pin="P6.2-/CS2-CC2IO" pad="9"/>
<connect gate="-BUS-INTERFACE" pin="P6.3-/CS3-CC3IO" pad="10"/>
<connect gate="-BUS-INTERFACE" pin="P6.4-/CS4-CC4IO" pad="11"/>
<connect gate="-BUS-INTERFACE" pin="P6.5-/HOLD-CC5IO" pad="12"/>
<connect gate="-BUS-INTERFACE" pin="P6.6-/HLDA-CC6IO" pad="13"/>
<connect gate="-BUS-INTERFACE" pin="P6.7-/BREQ-CC7IO" pad="14"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="/BRKIN" pad="144"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="/BRKOUT" pad="143"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="/TRST" pad="57"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="P3.15-CLKOUT-F" pad="77"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="TCK" pad="71"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="TDI" pad="72"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="TDO" pad="73"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="TMS-E*" pad="74"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="XTAL1" pad="138"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="XTAL2" pad="137"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="XTAL3" pad="140"/>
<connect gate="-CLOCK-JTAG-OCDSI" pin="XTAL4" pad="141"/>
<connect gate="-PORTS" pin="P2.10-CC10IO-EX2IN" pad="51"/>
<connect gate="-PORTS" pin="P2.11-CC11IO-EX3IN" pad="52"/>
<connect gate="-PORTS" pin="P2.12-CC12IO-EX4IN" pad="53"/>
<connect gate="-PORTS" pin="P2.13-CC13IO-EX5IN" pad="54"/>
<connect gate="-PORTS" pin="P2.14-CC14IO-EX6IN" pad="55"/>
<connect gate="-PORTS" pin="P2.15-CC15IO-EX7IN-T7IN" pad="56"/>
<connect gate="-PORTS" pin="P2.8-CC8IO-EX0IN" pad="49"/>
<connect gate="-PORTS" pin="P2.9-CC9IO-EX1IN" pad="50"/>
<connect gate="-PORTS" pin="P3.0-T0IN-TXD1-E*" pad="59"/>
<connect gate="-PORTS" pin="P3.1-T6OUT-RXD1-E*" pad="60"/>
<connect gate="-PORTS" pin="P3.10-TXD0-E*" pad="69"/>
<connect gate="-PORTS" pin="P3.11-RXD0-E*" pad="70"/>
<connect gate="-PORTS" pin="P3.13-SCLK0-E*" pad="76"/>
<connect gate="-PORTS" pin="P3.2-CAPIN" pad="61"/>
<connect gate="-PORTS" pin="P3.3-T3OUT" pad="62"/>
<connect gate="-PORTS" pin="P3.4-T3EUD" pad="63"/>
<connect gate="-PORTS" pin="P3.5-T4IN" pad="64"/>
<connect gate="-PORTS" pin="P3.6-T3IN" pad="65"/>
<connect gate="-PORTS" pin="P3.7-T2IN" pad="66"/>
<connect gate="-PORTS" pin="P3.8-MRST0" pad="67"/>
<connect gate="-PORTS" pin="P3.9-MTSR0" pad="68"/>
<connect gate="-PORTS" pin="P5.0-AN0" pad="29"/>
<connect gate="-PORTS" pin="P5.1-AN1" pad="30"/>
<connect gate="-PORTS" pin="P5.10-AN10-T6EUD" pad="35"/>
<connect gate="-PORTS" pin="P5.11-AN11-T5EUD" pad="36"/>
<connect gate="-PORTS" pin="P5.12-AN12-T6IN" pad="43"/>
<connect gate="-PORTS" pin="P5.13-AN13-T5IN" pad="44"/>
<connect gate="-PORTS" pin="P5.14-AN14-T4EUD" pad="45"/>
<connect gate="-PORTS" pin="P5.15-AN15-T2EUD" pad="46"/>
<connect gate="-PORTS" pin="P5.2-AN2" pad="31"/>
<connect gate="-PORTS" pin="P5.3-AN3" pad="32"/>
<connect gate="-PORTS" pin="P5.4-AN4" pad="33"/>
<connect gate="-PORTS" pin="P5.5-AN5" pad="34"/>
<connect gate="-PORTS" pin="P5.6-AN6" pad="39"/>
<connect gate="-PORTS" pin="P5.7-AN7" pad="40"/>
<connect gate="-PORTS" pin="P5.8-AN8" pad="37"/>
<connect gate="-PORTS" pin="P5.9-AN9" pad="38"/>
<connect gate="-PORTS" pin="P7.4-CC28IO-C*" pad="15"/>
<connect gate="-PORTS" pin="P7.5-CC29IO-C*" pad="16"/>
<connect gate="-PORTS" pin="P7.6-CC30IO-C*" pad="17"/>
<connect gate="-PORTS" pin="P7.7-CC31IO-C*" pad="18"/>
<connect gate="-PORTS" pin="P9.0-SDA0-CC16IO-C*" pad="21"/>
<connect gate="-PORTS" pin="P9.1-SCL0-CC17IO-C*" pad="22"/>
<connect gate="-PORTS" pin="P9.2-SDA1-CC18IO-C*" pad="23"/>
<connect gate="-PORTS" pin="P9.3-SCL1-CC19IO-C*" pad="24"/>
<connect gate="-PORTS" pin="P9.4-SDA2-CC20IO" pad="25"/>
<connect gate="-PORTS" pin="P9.5-SCL2-CC21IO" pad="26"/>
<connect gate="-PORTS" pin="VAGND" pad="42"/>
<connect gate="-PORTS" pin="VAREF" pad="41"/>
<connect gate="-POWER" pin="VDDI" pad="135"/>
<connect gate="-POWER" pin="VDDI@1" pad="78"/>
<connect gate="-POWER" pin="VDDI@2" pad="48"/>
<connect gate="-POWER" pin="VDDP" pad="125"/>
<connect gate="-POWER" pin="VDDP@1" pad="103"/>
<connect gate="-POWER" pin="VDDP@2" pad="88"/>
<connect gate="-POWER" pin="VDDP@3" pad="58"/>
<connect gate="-POWER" pin="VDDP@4" pad="28"/>
<connect gate="-POWER" pin="VDDP@5" pad="20"/>
<connect gate="-POWER" pin="VDDP@6" pad="6"/>
<connect gate="-POWER" pin="VSSI" pad="136"/>
<connect gate="-POWER" pin="VSSI@1" pad="139"/>
<connect gate="-POWER" pin="VSSI@2" pad="79"/>
<connect gate="-POWER" pin="VSSI@3" pad="47"/>
<connect gate="-POWER" pin="VSSP" pad="126"/>
<connect gate="-POWER" pin="VSSP@1" pad="104"/>
<connect gate="-POWER" pin="VSSP@2" pad="89"/>
<connect gate="-POWER" pin="VSSP@3" pad="27"/>
<connect gate="-POWER" pin="VSSP@4" pad="19"/>
<connect gate="-POWER" pin="VSSP@5" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
