<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Motorola pressure sensor&lt;/b&gt;&lt;p&gt;
SEMICONDUCTOR TECHNICAL DATA mpx2050.pdf</description>
<packages>
<package name="MPX2050DH">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
</package>
<package name="MPX2050DV">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
</package>
<package name="MPX2050GPH">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
</package>
<package name="MPX2050DPH">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
</package>
<package name="MPX2050DPV">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
</package>
<package name="MPX2050GPV">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
</package>
<package name="MPX2050GSXH">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
</package>
<package name="MPX2050GSXV">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
</package>
<package name="SOICW32">
<description>&lt;b&gt;Small Outline Package wide&lt;/b&gt;&lt;p&gt;
source www.motorola.com; BR1568.pdf</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; SO-8, CASE 751</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO24L">
<description>&lt;b&gt;Small Outline Package Large&lt;/b&gt; SO-24L; Case 751&lt;p&gt;
http://onsemi.com; mc33035-d.pdf</description>
</package>
<package name="DIL24S">
<description>&lt;b&gt;Dual In Line Small&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
<package name="SO20L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="HSOP">
<description>&lt;b&gt;Heatsink Small Outline Package (HSOP)&lt;/b&gt;&lt;p&gt;
Source: www.motorola.com/... AN2388.pdf</description>
</package>
</packages>
<symbols>
<symbol name="PRESS-SENSE">
<pin name="VS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="VO+" direction="pas"/>
<pin name="VO-" direction="pas"/>
</symbol>
<symbol name="PC33395">
<pin name="VIGN" direction="pwr"/>
<pin name="VGDH" direction="out"/>
<pin name="VIGNP" direction="pas"/>
<pin name="GDH1" direction="out"/>
<pin name="GDH2" direction="out"/>
<pin name="GDH3" direction="out"/>
<pin name="SRC1" direction="in"/>
<pin name="SRC2" direction="in"/>
<pin name="SRC3" direction="in"/>
<pin name="GDL1" direction="out"/>
<pin name="GDL2" direction="out"/>
<pin name="GDL3" direction="out"/>
<pin name="-ISENS" direction="in"/>
<pin name="+ISENS" direction="in"/>
<pin name="PGND" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="LSE1" direction="in"/>
<pin name="LSE2" direction="in"/>
<pin name="LSE3" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="HSE1" direction="in"/>
<pin name="HSE2" direction="in"/>
<pin name="HSE3" direction="in"/>
<pin name="CP1H" direction="pas"/>
<pin name="CP1L" direction="pas"/>
<pin name="CP2H" direction="pas"/>
<pin name="CP2L" direction="pas"/>
<pin name="CPRES" direction="pas"/>
<pin name="VDD" direction="pwr"/>
<pin name="PWM" direction="in"/>
<pin name="TEST" direction="in"/>
</symbol>
<symbol name="MC33039">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="!A" direction="out"/>
<pin name="RCT" direction="pas"/>
<pin name="FOUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MC33035">
<pin name="AT" direction="out"/>
<pin name="BT" direction="out"/>
<pin name="CT" direction="out"/>
<pin name="AB" direction="out"/>
<pin name="BB" direction="out"/>
<pin name="CB" direction="out"/>
<pin name="SA" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="SC" direction="in"/>
<pin name="REFO" direction="out"/>
<pin name="!FAULT" direction="out"/>
<pin name="ERROUT/!PWMIN" direction="pas"/>
<pin name="OE" direction="in"/>
<pin name="CSENSIN" direction="in"/>
<pin name="ERRAMP" direction="in"/>
<pin name="!ERRAMP" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="FWD/REV" direction="in"/>
<pin name="°60/!120" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="VC" direction="pwr"/>
<pin name="BRAKE" direction="in"/>
<pin name="!CSENSIN" direction="in"/>
</symbol>
<symbol name="MC33033">
<pin name="AT" direction="out"/>
<pin name="BT" direction="out"/>
<pin name="CT" direction="out"/>
<pin name="AB" direction="out"/>
<pin name="BB" direction="out"/>
<pin name="CB" direction="out"/>
<pin name="SA" direction="in"/>
<pin name="SB" direction="in"/>
<pin name="SC" direction="in"/>
<pin name="REFO" direction="out"/>
<pin name="ERROUT/!PWMIN" direction="pas"/>
<pin name="OE" direction="in"/>
<pin name="CSENSIN" direction="in"/>
<pin name="ERRAMP" direction="in"/>
<pin name="!ERRAMP" direction="in"/>
<pin name="OSC" direction="in"/>
<pin name="FWD/REV" direction="in"/>
<pin name="°60/!120" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MC33883">
<pin name="VCC2" direction="pwr"/>
<pin name="LR_OUT" direction="pas"/>
<pin name="GATE_HS2" direction="out"/>
<pin name="SRC_HS2" direction="out"/>
<pin name="GATE_LS2" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="LS1" direction="in"/>
<pin name="LS2" direction="in"/>
<pin name="HS1" direction="in"/>
<pin name="HS2" direction="in"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="EN" direction="in"/>
<pin name="GATE_HS1" direction="out"/>
<pin name="SRC_HS1" direction="out"/>
<pin name="GATE_LS1" direction="out"/>
<pin name="CP_OUT1" direction="pas"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND_A" direction="pwr"/>
</symbol>
<symbol name="SLUG">
<pin name="S" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MPX2050*" prefix="V">
<description>&lt;b&gt;50 kPa Pressure Sensor&lt;/b&gt;&lt;p&gt;
On-Chip Temparetur Compensated &amp; Calibrated Silicon Pressure Sensor</description>
<gates>
<gate name="G$1" symbol="PRESS-SENSE"/>
</gates>
<devices>
<device name="DH1" package="MPX2050DH">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VO+" pad="2"/>
<connect gate="G$1" pin="VO-" pad="4"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="DH3" package="MPX2050DH">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VO+" pad="4"/>
<connect gate="G$1" pin="VO-" pad="2"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="DV1" package="MPX2050DV">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VO+" pad="2"/>
<connect gate="G$1" pin="VO-" pad="4"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="DV3" package="MPX2050DV">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VO+" pad="4"/>
<connect gate="G$1" pin="VO-" pad="2"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="DPH" package="MPX2050DPH">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VO+" pad="2"/>
<connect gate="G$1" pin="VO-" pad="4"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="DPV" package="MPX2050DPV">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VO+" pad="2"/>
<connect gate="G$1" pin="VO-" pad="4"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MPX2050DP"/>
<attribute name="OC_FARNELL" value="3506642"/>
<attribute name="OC_NEWARK" value="48F6766"/>
</technology>
</technologies>
</device>
<device name="GPV" package="MPX2050GPV">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VO+" pad="2"/>
<connect gate="G$1" pin="VO-" pad="4"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="MOTOROLA"/>
<attribute name="MPN" value="MPX2050GP"/>
<attribute name="OC_FARNELL" value="8814910"/>
<attribute name="OC_NEWARK" value="48F6767"/>
</technology>
</technologies>
</device>
<device name="GPH" package="MPX2050DH">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VO+" pad="2"/>
<connect gate="G$1" pin="VO-" pad="4"/>
<connect gate="G$1" pin="VS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33395*" prefix="IC">
<description>&lt;b&gt;BLDC Motor Control, Three-Phase Gate Driver IC&lt;/b&gt;&lt;p&gt;
Source: http://www.freescale.com/files/analog/doc/data_sheet/MC33395.pdf</description>
<gates>
<gate name="G$1" symbol="PC33395"/>
</gates>
<devices>
<device name="WB" package="SOICW32">
<connects>
<connect gate="G$1" pin="+ISENS" pad="18"/>
<connect gate="G$1" pin="-ISENS" pad="17"/>
<connect gate="G$1" pin="AGND" pad="19"/>
<connect gate="G$1" pin="CP1H" pad="31"/>
<connect gate="G$1" pin="CP1L" pad="30"/>
<connect gate="G$1" pin="CP2H" pad="1"/>
<connect gate="G$1" pin="CP2L" pad="32"/>
<connect gate="G$1" pin="CPRES" pad="2"/>
<connect gate="G$1" pin="GDH1" pad="7"/>
<connect gate="G$1" pin="GDH2" pad="10"/>
<connect gate="G$1" pin="GDH3" pad="13"/>
<connect gate="G$1" pin="GDL1" pad="8"/>
<connect gate="G$1" pin="GDL2" pad="11"/>
<connect gate="G$1" pin="GDL3" pad="14"/>
<connect gate="G$1" pin="HSE1" pad="26"/>
<connect gate="G$1" pin="HSE2" pad="25"/>
<connect gate="G$1" pin="HSE3" pad="24"/>
<connect gate="G$1" pin="LSE1" pad="29"/>
<connect gate="G$1" pin="LSE2" pad="28"/>
<connect gate="G$1" pin="LSE3" pad="27"/>
<connect gate="G$1" pin="MODE0" pad="23"/>
<connect gate="G$1" pin="MODE1" pad="22"/>
<connect gate="G$1" pin="PGND" pad="15"/>
<connect gate="G$1" pin="PWM" pad="21"/>
<connect gate="G$1" pin="SRC1" pad="6"/>
<connect gate="G$1" pin="SRC2" pad="9"/>
<connect gate="G$1" pin="SRC3" pad="12"/>
<connect gate="G$1" pin="TEST" pad="16"/>
<connect gate="G$1" pin="VDD" pad="20"/>
<connect gate="G$1" pin="VGDH" pad="4"/>
<connect gate="G$1" pin="VIGN" pad="3"/>
<connect gate="G$1" pin="VIGNP" pad="5"/>
</connects>
<technologies>
<technology name="D">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="TD">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MC33395TEW"/>
<attribute name="OC_FARNELL" value="1380046"/>
<attribute name="OC_NEWARK" value="81K2764"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*33039" prefix="IC">
<description>&lt;b&gt;Closed Loop Brushless Motor Adapter&lt;/b&gt;&lt;p&gt;
*NCV33039: Tlow = -40C, Thigh = +125C. Guaranteed by design.&lt;br&gt;
http://onsemi.com; mc33039-d.pdf</description>
<gates>
<gate name="G$1" symbol="MC33039"/>
</gates>
<devices>
<device name="D" package="SO08">
<connects>
<connect gate="G$1" pin="!A" pad="4"/>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="FOUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RCT" pad="6"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="MC">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC33039D"/>
<attribute name="OC_FARNELL" value="1150437"/>
<attribute name="OC_NEWARK" value="07F4700"/>
</technology>
<technology name="NCV">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="NCV33039DR2G"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="42K2044"/>
</technology>
</technologies>
</device>
<device name="P" package="DIP08">
<connects>
<connect gate="G$1" pin="!A" pad="4"/>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
<connect gate="G$1" pin="FOUT" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="RCT" pad="6"/>
<connect gate="G$1" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name="MC">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC33039P"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="07F4701"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*33035" prefix="IC">
<description>&lt;b&gt;Brushless DC Motor Controller&lt;/b&gt;&lt;p&gt;
http://onsemi.com; mc33035-d.pdf</description>
<gates>
<gate name="G$1" symbol="MC33035"/>
</gates>
<devices>
<device name="DW" package="SO24L">
<connects>
<connect gate="G$1" pin="!CSENSIN" pad="15"/>
<connect gate="G$1" pin="!ERRAMP" pad="12"/>
<connect gate="G$1" pin="!FAULT" pad="14"/>
<connect gate="G$1" pin="AB" pad="21"/>
<connect gate="G$1" pin="AT" pad="2"/>
<connect gate="G$1" pin="BB" pad="20"/>
<connect gate="G$1" pin="BRAKE" pad="23"/>
<connect gate="G$1" pin="BT" pad="1"/>
<connect gate="G$1" pin="CB" pad="19"/>
<connect gate="G$1" pin="CSENSIN" pad="9"/>
<connect gate="G$1" pin="CT" pad="24"/>
<connect gate="G$1" pin="ERRAMP" pad="11"/>
<connect gate="G$1" pin="ERROUT/!PWMIN" pad="13"/>
<connect gate="G$1" pin="FWD/REV" pad="3"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="OE" pad="7"/>
<connect gate="G$1" pin="OSC" pad="10"/>
<connect gate="G$1" pin="REFO" pad="8"/>
<connect gate="G$1" pin="SA" pad="4"/>
<connect gate="G$1" pin="SB" pad="5"/>
<connect gate="G$1" pin="SC" pad="6"/>
<connect gate="G$1" pin="VC" pad="18"/>
<connect gate="G$1" pin="VCC" pad="17"/>
<connect gate="G$1" pin="°60/!120" pad="22"/>
</connects>
<technologies>
<technology name="MC">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC33035DW"/>
<attribute name="OC_FARNELL" value="1652428"/>
<attribute name="OC_NEWARK" value="07F4697"/>
</technology>
<technology name="NCV">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="NCV33035DWR2"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="67C3170"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL24S">
<connects>
<connect gate="G$1" pin="!CSENSIN" pad="15"/>
<connect gate="G$1" pin="!ERRAMP" pad="12"/>
<connect gate="G$1" pin="!FAULT" pad="14"/>
<connect gate="G$1" pin="AB" pad="21"/>
<connect gate="G$1" pin="AT" pad="2"/>
<connect gate="G$1" pin="BB" pad="20"/>
<connect gate="G$1" pin="BRAKE" pad="23"/>
<connect gate="G$1" pin="BT" pad="1"/>
<connect gate="G$1" pin="CB" pad="19"/>
<connect gate="G$1" pin="CSENSIN" pad="9"/>
<connect gate="G$1" pin="CT" pad="24"/>
<connect gate="G$1" pin="ERRAMP" pad="11"/>
<connect gate="G$1" pin="ERROUT/!PWMIN" pad="13"/>
<connect gate="G$1" pin="FWD/REV" pad="3"/>
<connect gate="G$1" pin="GND" pad="16"/>
<connect gate="G$1" pin="OE" pad="7"/>
<connect gate="G$1" pin="OSC" pad="10"/>
<connect gate="G$1" pin="REFO" pad="8"/>
<connect gate="G$1" pin="SA" pad="4"/>
<connect gate="G$1" pin="SB" pad="5"/>
<connect gate="G$1" pin="SC" pad="6"/>
<connect gate="G$1" pin="VC" pad="18"/>
<connect gate="G$1" pin="VCC" pad="17"/>
<connect gate="G$1" pin="°60/!120" pad="22"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC33035P"/>
<attribute name="OC_FARNELL" value="1192056"/>
<attribute name="OC_NEWARK" value="07F4698"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="*33033" prefix="IC">
<description>&lt;b&gt;Brushless DC Motor Controller&lt;/b&gt;&lt;p&gt;
http://onsemi.com; mc33033-d.pdf</description>
<gates>
<gate name="G$1" symbol="MC33033"/>
</gates>
<devices>
<device name="P" package="DIL20">
<connects>
<connect gate="G$1" pin="!ERRAMP" pad="10"/>
<connect gate="G$1" pin="AB" pad="17"/>
<connect gate="G$1" pin="AT" pad="2"/>
<connect gate="G$1" pin="BB" pad="16"/>
<connect gate="G$1" pin="BT" pad="1"/>
<connect gate="G$1" pin="CB" pad="15"/>
<connect gate="G$1" pin="CSENSIN" pad="12"/>
<connect gate="G$1" pin="CT" pad="20"/>
<connect gate="G$1" pin="ERRAMP" pad="9"/>
<connect gate="G$1" pin="ERROUT/!PWMIN" pad="11"/>
<connect gate="G$1" pin="FWD/REV" pad="3"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="OE" pad="19"/>
<connect gate="G$1" pin="OSC" pad="8"/>
<connect gate="G$1" pin="REFO" pad="7"/>
<connect gate="G$1" pin="SA" pad="4"/>
<connect gate="G$1" pin="SB" pad="5"/>
<connect gate="G$1" pin="SC" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="°60/!120" pad="18"/>
</connects>
<technologies>
<technology name="MC">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC33033P"/>
<attribute name="OC_FARNELL" value="702857"/>
<attribute name="OC_NEWARK" value="07F4693"/>
</technology>
</technologies>
</device>
<device name="DW" package="SO20L">
<connects>
<connect gate="G$1" pin="!ERRAMP" pad="10"/>
<connect gate="G$1" pin="AB" pad="17"/>
<connect gate="G$1" pin="AT" pad="2"/>
<connect gate="G$1" pin="BB" pad="16"/>
<connect gate="G$1" pin="BT" pad="1"/>
<connect gate="G$1" pin="CB" pad="15"/>
<connect gate="G$1" pin="CSENSIN" pad="12"/>
<connect gate="G$1" pin="CT" pad="20"/>
<connect gate="G$1" pin="ERRAMP" pad="9"/>
<connect gate="G$1" pin="ERROUT/!PWMIN" pad="11"/>
<connect gate="G$1" pin="FWD/REV" pad="3"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="OE" pad="19"/>
<connect gate="G$1" pin="OSC" pad="8"/>
<connect gate="G$1" pin="REFO" pad="7"/>
<connect gate="G$1" pin="SA" pad="4"/>
<connect gate="G$1" pin="SB" pad="5"/>
<connect gate="G$1" pin="SC" pad="6"/>
<connect gate="G$1" pin="VCC" pad="14"/>
<connect gate="G$1" pin="°60/!120" pad="18"/>
</connects>
<technologies>
<technology name="MC">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="MC33033DW"/>
<attribute name="OC_FARNELL" value="1364058"/>
<attribute name="OC_NEWARK" value="07F4692"/>
</technology>
<technology name="NCV">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="NCV33033DWR2"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="67C3169"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MC33883" prefix="IC">
<description>&lt;b&gt;Full Bridge Pre-Driver&lt;/b&gt; 55V&lt;p&gt;
Source: www.motorola.com/... MC33883.pdf</description>
<gates>
<gate name="G$1" symbol="MC33883"/>
</gates>
<devices>
<device name="DW" package="SO20L">
<connects>
<connect gate="G$1" pin="C1" pad="13"/>
<connect gate="G$1" pin="C2" pad="2"/>
<connect gate="G$1" pin="CP_OUT1" pad="3"/>
<connect gate="G$1" pin="EN" pad="20"/>
<connect gate="G$1" pin="GATE_HS1" pad="5"/>
<connect gate="G$1" pin="GATE_HS2" pad="18"/>
<connect gate="G$1" pin="GATE_LS1" pad="8"/>
<connect gate="G$1" pin="GATE_LS2" pad="15"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="14"/>
<connect gate="G$1" pin="GND_A" pad="12"/>
<connect gate="G$1" pin="HS1" pad="6"/>
<connect gate="G$1" pin="HS2" pad="17"/>
<connect gate="G$1" pin="LR_OUT" pad="10"/>
<connect gate="G$1" pin="LS1" pad="7"/>
<connect gate="G$1" pin="LS2" pad="16"/>
<connect gate="G$1" pin="SRC_HS1" pad="4"/>
<connect gate="G$1" pin="SRC_HS2" pad="19"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
