<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>Murata Rotary Position Sensor</description>
<packages>
<package name="SV01A">
<description>&lt;b&gt;Rotary Position Sensors&lt;/b&gt;&lt;p&gt;
SMD/Lead Dust-proof Type 12mm Size SV01 Series&lt;br&gt;
Source: http://www.murata.com/catalog/r50/el0595.pdf</description>
</package>
<package name="SV01L">
<description>&lt;b&gt;Rotary Position Sensors&lt;/b&gt;&lt;p&gt;
SMD/Lead Dust-proof Type 12mm Size SV01 Series&lt;br&gt;
Source: http://www.murata.com/catalog/r50/el0595.pdf</description>
</package>
</packages>
<symbols>
<symbol name="ROT_POS_SENSOR">
<pin name="+V" direction="pas"/>
<pin name="-V" direction="pas"/>
<pin name="OUT" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="SV01" prefix="SN">
<description>&lt;b&gt;Rotary Position Sensors&lt;/b&gt;&lt;p&gt;
SMD/Lead Dust-proof Type 12mm Size SV01 Series&lt;br&gt;
Source: http://www.murata.com/catalog/r50/el0595.pdf</description>
<gates>
<gate name="G$1" symbol="ROT_POS_SENSOR"/>
</gates>
<devices>
<device name="A" package="SV01A">
<connects>
<connect gate="G$1" pin="+V" pad="3"/>
<connect gate="G$1" pin="-V" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1406648"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="SV01L">
<connects>
<connect gate="G$1" pin="+V" pad="3"/>
<connect gate="G$1" pin="-V" pad="1"/>
<connect gate="G$1" pin="OUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
