<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<library>
<description>ALPS Switch from Markus Faust &amp;lt;mfaust@htwm.de&amp;gt;&lt;p&gt;
Source: EC12E.scr from eagle.support.ger on news.cadsoft.de at 08.10.2007</description>
<packages>
<package name="ALPS_EC12E_SW">
<description>ALPS rotary encoder&lt;br&gt;
EC12E series with push-on switch</description>
</package>
</packages>
<symbols>
<symbol name="ENCODER">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="TASTER">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="GEHAEUSEANSCHLUSS">
<pin name="G" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="EC12E_SW" prefix="SW">
<description>ALPS rotary Encoder EC12E series with switch</description>
<gates>
<gate name="G$1" symbol="ENCODER"/>
<gate name="G$2" symbol="TASTER"/>
<gate name="G$3" symbol="GEHAEUSEANSCHLUSS"/>
<gate name="G$4" symbol="GEHAEUSEANSCHLUSS"/>
</gates>
<devices>
<device name="" package="ALPS_EC12E_SW">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$2" pin="1" pad="D"/>
<connect gate="G$2" pin="2" pad="E"/>
<connect gate="G$3" pin="G" pad="GND1"/>
<connect gate="G$4" pin="G" pad="GND2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EC12E2424407"/>
<attribute name="OC_FARNELL" value="1520813"/>
<attribute name="OC_NEWARK" value="74M1068"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
