<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;to telecontrolli&lt;/b&gt; RF Receivers, RF Transmitters, RF Transceivers&lt;p&gt;
Thick Film Hybrid Technology&lt;p&gt;
Via Naz. delle Puglie, 177&lt;br&gt;
80026 CASORIA (NA), Italy&lt;br&gt;
Tel: +39 081 7599033&lt;br&gt;
http://www.telecontrolli.com/eng/default.html</description>
<packages>
<package name="RRFQ1">
<description>&lt;b&gt;Ceramic Hybrid Package&lt;/b&gt;&lt;p&gt;
Source: http://www.telecontrolli.com/eng/default-wproducts.html ... rrfq1.pdf</description>
</package>
<package name="RTFQ2">
<description>&lt;b&gt;Ceramic Hybrid Package&lt;/b&gt;&lt;p&gt;
Source: http://www.telecontrolli.com/eng/default-wproducts.html ... rtfq2.pdf</description>
</package>
<package name="RXQ1">
<description>&lt;b&gt;RXQ1-433.9 Dual Band FM Transceiver&lt;/b&gt;&lt;p&gt;
Source: http://www.telecontrolli.com/pdf/transceivers/RXQ1.pdf</description>
</package>
</packages>
<symbols>
<symbol name="RRFQ1">
<pin name="+5V" direction="pwr"/>
<pin name="RSSI" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="PD" direction="in"/>
</symbol>
<symbol name="RTFQ2">
<pin name="+5V" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="IN" direction="in"/>
<pin name="EA" direction="out"/>
</symbol>
<symbol name="RXQ1">
<pin name="RF_GND@1" direction="pwr"/>
<pin name="ANT" direction="in"/>
<pin name="RF_GND@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="RXD" direction="out"/>
<pin name="TXD" direction="in"/>
<pin name="!TXSELECT" direction="in"/>
<pin name="!RXSELECT" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="CS" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RRFQ1-*" prefix="HY">
<description>&lt;b&gt;FSK Superhet Receiver with Crystal Oscillator&lt;/b&gt;&lt;p&gt;
Source: http://www.telecontrolli.com/eng/default-wproducts.html ... rrfq1.pdf</description>
<gates>
<gate name="G$1" symbol="RRFQ1"/>
</gates>
<devices>
<device name="" package="RRFQ1">
<connects>
<connect gate="G$1" pin="+5V" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="GND@1" pad="7"/>
<connect gate="G$1" pin="GND@2" pad="11"/>
<connect gate="G$1" pin="IN" pad="3"/>
<connect gate="G$1" pin="OUT" pad="14"/>
<connect gate="G$1" pin="PD" pad="15"/>
<connect gate="G$1" pin="RSSI" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="FM-RRFQ1-868"/>
<attribute name="OC_FARNELL" value="1201003"/>
<attribute name="OC_NEWARK" value="01M7854"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTFQ2-*" prefix="HY">
<description>&lt;b&gt;FSK Radio Transmitter with Crystal Oscillator and External Antenna&lt;/b&gt;&lt;p&gt;
Source: http://www.telecontrolli.com/eng/default-wproducts.html ... rtfq2.pdf</description>
<gates>
<gate name="G$1" symbol="RTFQ2"/>
</gates>
<devices>
<device name="" package="RTFQ2">
<connects>
<connect gate="G$1" pin="+5V" pad="10"/>
<connect gate="G$1" pin="EA" pad="2"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND@1" pad="11"/>
<connect gate="G$1" pin="IN" pad="12"/>
</connects>
<technologies>
<technology name="315">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="433.92">
<attribute name="MF" value=""/>
<attribute name="MPN" value="FM-RTFQ2-433R"/>
<attribute name="OC_FARNELL" value="1200990"/>
<attribute name="OC_NEWARK" value="01M7858"/>
</technology>
<technology name="868.35">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RXQ1*" prefix="HY">
<description>&lt;b&gt;RXQ1-433.9 Dual Band FM Transceiver&lt;/b&gt;&lt;p&gt;
Source: http://www.telecontrolli.com/pdf/transceivers/RXQ1.pdf</description>
<gates>
<gate name="G$1" symbol="RXQ1"/>
</gates>
<devices>
<device name="" package="RXQ1">
<connects>
<connect gate="G$1" pin="!RXSELECT" pad="16"/>
<connect gate="G$1" pin="!TXSELECT" pad="15"/>
<connect gate="G$1" pin="ANT" pad="2"/>
<connect gate="G$1" pin="CS" pad="18"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="9"/>
<connect gate="G$1" pin="GND@3" pad="10"/>
<connect gate="G$1" pin="RF_GND@1" pad="1"/>
<connect gate="G$1" pin="RF_GND@2" pad="3"/>
<connect gate="G$1" pin="RXD" pad="12"/>
<connect gate="G$1" pin="TXD" pad="14"/>
<connect gate="G$1" pin="VCC" pad="17"/>
</connects>
<technologies>
<technology name="-433.9">
<attribute name="MF" value=""/>
<attribute name="MPN" value="FM-RXQ1-433"/>
<attribute name="OC_FARNELL" value="1200988"/>
<attribute name="OC_NEWARK" value="96K9948"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
