<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<library>
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TVSOP48">
<description>&lt;b&gt;Plastic Small Outline&lt;/b&gt;</description>
</package>
<package name="PQFP144">
<description>&lt;b&gt;Platic Quad Flat Package&lt;/b&gt;&lt;p&gt;
PGE (S-PQFP-G144)</description>
</package>
<package name="SO-16DW">
<description>&lt;b&gt;DW (RPDSO-G16)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/iso1176.pdf</description>
</package>
<package name="PQFP48">
<description>&lt;b&gt;Platic Quad Flat Package&lt;/b&gt;</description>
</package>
<package name="SO-20DW">
<description>&lt;b&gt;Small Outline Integrated Circuit&lt;/b&gt; wide</description>
</package>
<package name="TSSOP8">
<description>&lt;b&gt;Plastic Small Outline&lt;/b&gt;</description>
</package>
<package name="SO-16">
<description>&lt;b&gt;Small Outline Integrated Circuit&lt;/b&gt;</description>
</package>
<package name="SO-08">
<description>&lt;b&gt;D (R-PDSO-G8)&lt;/b&gt; Plastic Small Outline Package&lt;p&gt;

Source: http://focus.ti.com/lit/ds/symlink/sn65als176.pdf</description>
</package>
<package name="PLCC20">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt;</description>
</package>
<package name="SO-18DW">
<description>&lt;b&gt;Small Outline Integrated Circuit&lt;/b&gt; wide</description>
</package>
<package name="SO-14DW">
<description>&lt;b&gt;Small Outline Integrated Circuit&lt;/b&gt; wide</description>
</package>
<package name="DIL08-OPTO">
<description>&lt;b&gt;Dula In Line&lt;/b&gt;&lt;p&gt;
This dual-in-line package consists of an integrated circuit mounted on a lead frame and encapsulated with an
electrically nonconductive clear plastic compound. The photodiode area is typically 1.36 mm2&lt;p&gt;
from tsl230.pdf TAOS004 - MAY 1999</description>
</package>
<package name="DDPACK-7">
<description>&lt;b&gt;PLASTIC FLANGE-MOUNT&lt;/b&gt;</description>
</package>
<package name="SSOP28DL">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="SSOP20">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="PSO28">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt;&lt;p&gt;
PW (R-PDSO-G**)&lt;br&gt;
www.ti.com; tas3001.pdf</description>
</package>
<package name="PBGA144">
<description>&lt;b&gt;PLASTIC BALL GRID ARRAY PACKAGE&lt;/b&gt;&lt;p&gt;
GGU (S-PBGA-N144) Source: tms320vc5402.pdf</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="D_R-PDSO-G14">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 14&lt;/b&gt; JEDEC MS-012, D Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="PW_R-PDSO-G08">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE, SO 8&lt;/b&gt; JEDEC MO-153, PW Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="D_R-PDSO-G16">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 16&lt;/b&gt; JEDEC MS-012, D Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="PW_R-PDSO-G20">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 20&lt;/b&gt; JEDEC MO-153, PW Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="PW_R-PDSO-G24">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 24&lt;/b&gt; JEDEC MO-153, PW Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="PW_R-PDSO-G28">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 28&lt;/b&gt; JEDEC MO-153, PW Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="SQFP-S-10X10-64">
<description>&lt;b&gt;QFP64&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="HTSSOP20PWP">
<description>&lt;b&gt;TPS40055PWP&lt;/b&gt; (R-PDSO-G**) PowerPAD (TM) 20 pol.&lt;p&gt;
PLASTIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: www.ti.com ... TPS40055 package.pdf &amp; slma002.pdf</description>
</package>
<package name="HTSSOP24PWP">
<description>&lt;b&gt;TPS40055PWP&lt;/b&gt; (R-PDSO-G**) PowerPAD (TM) 24 pol.&lt;p&gt;
PLASTIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: www.ti.com ... TPS40055 package.pdf &amp; slma002.pdf</description>
</package>
<package name="HTSSOP28PWP">
<description>&lt;b&gt;TPS40055PWP&lt;/b&gt; (R-PDSO-G**) PowerPAD (TM) 28 pol.&lt;p&gt;
PLASTIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: www.ti.com ... TPS40055 package.pdf &amp; slma002.pdf</description>
</package>
<package name="HTSSOP16PWP">
<description>&lt;b&gt;TPS40055PWP&lt;/b&gt; (R-PDSO-G**) PowerPAD (TM) 16 pol.&lt;p&gt;
PLASTIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: www.ti.com ... TPS40055 package.pdf &amp; slma002.pdf</description>
</package>
<package name="HTSSOP14PWP">
<description>&lt;b&gt;TPS40055PWP&lt;/b&gt; (R-PDSO-G**) PowerPAD (TM) 14 pol.&lt;p&gt;
PLASTIC SMALL-OUTLINE PACKAGE&lt;br&gt;
Source: www.ti.com ... TPS40055 package.pdf &amp; slma002.pdf</description>
</package>
<package name="HTQFP-64-EXP">
<description>&lt;b&gt;TQFP 64 PowerPAD Package&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. slma002.pdf</description>
</package>
<package name="HTQFP-64-PAP">
<description>&lt;b&gt;PAP (S-PQFP-G46)&lt;/b&gt; PowerPAD Package&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1274.pdf&lt;br&gt;
www.ti.com .. slma002.pdf</description>
</package>
<package name="HTSSOP48DHD">
<description>&lt;b&gt;PowerPAD (TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DHD (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds038/mpds038.pdf</description>
</package>
<package name="HTSSOP56DCA">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DCA (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds044/mpds044.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP64DCA">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DCA (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds044/mpds044.pdf</description>
</package>
<package name="HTSSOP48DCA">
<description>&lt;b&gt;PowerPADE PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt;&lt;p&gt;
DCA (R-PDSO-G**)&lt;br&gt;
Source: http://focus.ti.com/lit/ml/mpds044/mpds044.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP56DHD">
<description>&lt;b&gt;PowerPAD (TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DHD (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds038/mpds038.pdf</description>
</package>
<package name="HTSSOP64DFD">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DFD (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds045b/mpds045b.pdf</description>
</package>
<package name="HTSSOP56DFD">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DFD (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds045b/mpds045b.pdf</description>
</package>
<package name="HTSSOP48DFD">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DFD (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds045b/mpds045b.pdf</description>
</package>
<package name="HTSSOP28DCP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DCP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds041b/mpds041b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP28DAP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DAP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds029b/mpds029b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP30DAP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DAP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds029b/mpds029b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP32DAP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DAP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds029b/mpds029b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP38DAP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DAP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds029b/mpds029b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP8DGN">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DGN (R-PDSO-G8)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds046b/mpds046b.pdf</description>
</package>
<package name="HTSSOP30DCP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DCP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds041b/mpds041b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP38DCP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DCP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds041b/mpds041b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP44DCP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DCP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds041b/mpds041b.pdf / slma002.pdf</description>
</package>
<package name="HTSSOP50DCP">
<description>&lt;b&gt;PowerPAD(TM) PLASTIC SMALL-OUTLINE PACKAGE&lt;/b&gt; DCP (R-PDSO-G**)&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds041b/mpds041b.pdf / slma002.pdf</description>
</package>
<package name="S-PDSO-G08">
<description>DGN (S-PDSO-G8) PowerPAD (TM) Plastic Small-Outline Package&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ths4211.pdf</description>
</package>
<package name="R-PSOP-G24">
<description>&lt;b&gt;DCV (R-PSOP-G24)&lt;/b&gt; PLASTIC SMALL-OUTLINE&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm3006.pdf</description>
</package>
<package name="R-PQFP-N20">
<description>&lt;b&gt;PQFP20&lt;/b&gt; RHL PACKAGE 4.5mm x 3.5mm QFN&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps75003.pdf</description>
</package>
<package name="PLCC68S">
<description>&lt;b&gt;PLASTIC LEADED CHIP CARRIER&lt;/b&gt;&lt;p&gt;
square</description>
</package>
<package name="TSOT23-6_DDC">
<description>&lt;b&gt;DDC (R-PDSO-G6)&lt;/b&gt; PLASTIC SMALL OUTLINE PACKAGE&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps61070.pdf</description>
</package>
<package name="PBGA-N64">
<description>&lt;b&gt;GXG (S-PBGA-N64&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ddc232.pdf</description>
</package>
<package name="S-PDSO-N10">
<description>&lt;b&gt;QFN 10&lt;/b&gt; 3 x 3 mm&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps61200.pdf</description>
</package>
<package name="TQFP100">
<description>&lt;b&gt;PLASTIC 100-PIN TQFP&lt;/b&gt; (PZ)&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 19&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/docs/prod/folders/print/msp430fg4618.html</description>
</package>
<package name="S-PBGA-N113">
<description>&lt;b&gt;PLASTIC BGA 113-BALL&lt;/b&gt; (ZQW)&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 19&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/docs/prod/folders/print/msp430fg4618.html</description>
</package>
<package name="DCK">
<description>&lt;b&gt;DCK R-PDSO-G5&lt;/b&gt; 5-Pin SC-70 Package (SOT323)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps3803-01.pdf</description>
</package>
<package name="SOP-08">
<description>&lt;b&gt;PS (R-PDSO-G8)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com .. sn65176b.pdf</description>
</package>
<package name="CBB">
<description>&lt;b&gt;CBB (S-PBGA-N515)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 23&lt;/i&gt;&lt;br&gt;
Source: sprm315.bsd</description>
</package>
<package name="CUS">
<description>&lt;b&gt;CUS (S-PBGA-N423)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 23&lt;/i&gt;&lt;br&gt;
Source: sprm314.bsd</description>
</package>
<package name="QFN40-6X6">
<description>&lt;b&gt;RHA (S-PQFP-N40) 6 x 6 mm&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps65020.pdf</description>
</package>
<package name="QFN40-5X5">
<description>&lt;b&gt;RSB (S-PWQFN-N40)&lt;/b&gt;&lt;p&gt;
Set restring parameter in design rules to 0, for top, inner, bottom at minimum and %.&lt;br&gt;
Source: RSB_TPS65023RSB_Land_Pattern.pdf</description>
</package>
<package name="QFN20_3,5X4,5">
<description>&lt;b&gt;RHL (R-PQFP-N20)&lt;/b&gt;&lt;p&gt;
Set in DRC - Same Signals - SMD to SMD and SMD to PAD = 0.&lt;br&gt;
Source: www.ti.com .. TI-bq24125.pdf</description>
</package>
<package name="DRZ">
<description>&lt;b&gt;DRZ (S-PDSO-N12) PLASTIC SMALL OUTLINE&lt;/b&gt;&lt;p&gt;
Source: bq27500-v100.pdf</description>
</package>
<package name="SOT23-DBV">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; DBV (R-PDSO-G5)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps77001.pdf</description>
</package>
<package name="DRK_S-PDSO-N10">
<description>&lt;b&gt;DRK (S-PDSO-N10)&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. bq27010.pdf</description>
</package>
<package name="D_R-PDSO-G08">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 14&lt;/b&gt; JEDEC MS-012, D Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="PW_R-PDSO-G16">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 16&lt;/b&gt; JEDEC MO-153, PW Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="PW_R-PDSO-G14">
<description>&lt;b&gt;PLASTIC SMALL-OUTLINE PACKAGE SO 14&lt;/b&gt; JEDEC MO-153, PW Type&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
</package>
<package name="DBZ_R-PDSO-G3">
<description>&lt;b&gt;DBZ (R-PDSO-G3)&lt;/b&gt; SOT-23&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slcs146e/slcs146e.pdf</description>
</package>
<package name="DCK_R-PDSO-G5">
<description>&lt;b&gt;DCK (R-PDSO-G5)&lt;/b&gt; SC-70&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slcs146e/slcs146e.pdf</description>
</package>
<package name="LP_O-PBCY-W3">
<description>&lt;b&gt;LP (O-PBCY-W3)&lt;/b&gt; TO-92/TO-226&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slcs146e/slcs146e.pdf</description>
</package>
<package name="PZ_S-PQFP-G100">
<description>&lt;b&gt;QFP100&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. msp430f5437.pdf</description>
</package>
<package name="PN_S-PQFP-G80">
<description>&lt;b&gt;QFP80&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. msp430f5437.pdf</description>
</package>
<package name="TSSOP38_R-PDSO-G38-DA">
<description>&lt;b&gt;TSSOP 38&lt;/b&gt; DA (R-PDSO-G38)&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 28&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/msp430f2274.pdf</description>
</package>
<package name="DGK-R-PDSO-G8">
<description>&lt;B&gt;DGK (R-PDSO-G8)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps77333.pdf</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="QFN16">
<description>&lt;b&gt;RTE (S-PQFP-N16)&lt;/b&gt; 3x3 mm&lt;p&gt;
Source: www.ti.com .. tpa6132a2 direct path stereo $.65.pdf</description>
</package>
<package name="PWP-TSSOP24">
<description>&lt;b&gt;PWP (R-PDSO-G24) PowerPAD&lt;/b&gt; TM&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tpa3123d2.pdf</description>
</package>
<package name="S-PQFP-G48">
<description>&lt;b&gt;PFB (S-PQFP-G48)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/src4392.pdf</description>
</package>
<package name="ZDH_S-PBGA-N256">
<description>&lt;b&gt;ZDH (S-PBGA-N256)&lt;/b&gt; PLASTIC BALL GRID ARRAY&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tms320c6720.pdf</description>
</package>
<package name="GDH_S-PBGA-N256">
<description>&lt;b&gt;GDH (S-PBGA-N256)&lt;/b&gt; PLASTIC BALL GRID ARRAY&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tms320c6720.pdf</description>
</package>
<package name="RFP_S-PQFP-G144-EXPAD">
<description>&lt;b&gt;RFP_S-PQFP-G144&lt;/b&gt; PowerPAD PLASTIC QUAD FLATPACK&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tms320c6720.pdf&lt;br&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="RFP_S-PQFP-G144-EXP">
<description>&lt;b&gt;RFP (S-PQFP-G144) PowerPAD TM&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tms320c6720.pdf</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;PW (R-PDSO-G8)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1271.pdf</description>
</package>
<package name="DUB-R-PDSO-G8">
<description>&lt;b&gt;DUB (R-PDSO-G8)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/iso1050.pdf</description>
</package>
<package name="PDIP-T28">
<description>&lt;b&gt;NT (R-PDIP-T28)&lt;/b&gt; PLASTIC DUAL-IN-LINE PACKAGE&lt;/b&gt;
Source: http://focus.ti.com/lit/ml/mpdi004a/mpdi004a.pdf</description>
</package>
<package name="PDIP-T24">
<description>&lt;b&gt;NT (R-PDIP-T24)&lt;/b&gt; PLASTIC DUAL-IN-LINE PACKAGE&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpdi004a/mpdi004a.pdf</description>
</package>
<package name="DB_R-PDSO-G28">
<description>&lt;b&gt;DB (R-PDSO-G28)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1210.pdf</description>
</package>
<package name="ZKB_S-PBGA-N256">
<description>&lt;b&gt;sprm328&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: sprm328.bsm</description>
</package>
<package name="GTS_S-PBGA-N288">
<description>&lt;b&gt;Flip Chip BGA Package&lt;/b&gt; GTS (S-PBGA-N288)&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: sprm148b.bsd&lt;br&gt;
http://focus.ti.com/lit/ug/spru811a/spru811a.pdf</description>
</package>
<package name="ZUN_SPBGA-N561">
<description>&lt;b&gt;ZUN (S-PBGA-N561)&lt;/b&gt; OLASTIC BALL GRID ARRAY&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: sprm335.bsd&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/tms320c6474.pdf</description>
</package>
<package name="DKD_R-PDSO-G36">
<description>&lt;b&gt;Thermally-enhanced 36-pin PSOP3 PowerPAD(TM) package&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tas5261.pdf</description>
</package>
<package name="DGK_S-PDSO-G8">
<description>8-Pin MSOP (DGK) Package&lt;p&gt;
Source:
&lt;a href="http://www.ti.com/lit/ml/mpds028d/mpds028d.pdf")&gt; DGK (S-PDSO-G8)&lt;/a&gt;
&lt;/p&gt;</description>
</package>
<package name="PFB_S-PQFP-G48">
<description>&lt;b&gt;PFB (S-PQFP-G48)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm4220.pdf</description>
</package>
<package name="PAP_S-PQFP-G64">
<description>&lt;b&gt;PAP (S-PQFP-G64) PowerPAD (TM)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm4204.pdf</description>
</package>
<package name="DBT_R-PDSO-G38">
<description>&lt;b&gt;DBT (R-PSDO-G38)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpds019g/mpds019g.pdf</description>
</package>
<package name="ZCE_S-PBGA-N361">
<description>&lt;b&gt;ZCE (S-PBGA-N361)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Source: sprm377a.bsm&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/omap-l138.pdf</description>
</package>
<package name="ZWT_S-PBGA-N361">
<description>&lt;b&gt;ZWT (S-PBGA-N361)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Source: sprm376a.bsm&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/omap-l138.pdf</description>
</package>
<package name="ZEN_S-PBGA-N196">
<description>&lt;b&gt;ZEN (S-PBGA-N196)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ml/mpbg838/mpbg838.pdf</description>
</package>
<package name="GHH_S-PBGA-N179">
<description>&lt;b&gt;GHH (S-PBGA-N179)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Source: sprm155a.bsm&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/tms320vc5509a.pdf</description>
</package>
<package name="VF_S-PQFP-G32">
<description>&lt;b&gt;VF (S-PQFP-G32)&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Souirce: http://focus.ti.com/lit/ds/symlink/tusb2046b.pdf</description>
</package>
<package name="RHB_S-PQFP-N32">
<description>&lt;b&gt;RHB (S-PQFP-N32)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tusb2046b.pdf</description>
</package>
<package name="DL_R-PDSO-G48">
<description>&lt;b&gt;DL_R-PDSO-G48&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="RGC_S-PVQFV-N64">
<description>&lt;b&gt;RGC(S-PVQFN-N64)&lt;/b&gt; CUSTOM DEVICE PASTRIC QUAD FLATPACK NO-LEAD&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/msp430f2471.pdf</description>
</package>
<package name="75ALS176">
<description>&lt;b&gt;&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="DDC232">
<description>&lt;b&gt;&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 34&lt;/i&gt;&lt;br&gt;</description>
</package>
<package name="RHA_S-PVQFN-N40">
<description>&lt;b&gt;RHA (S-PVQFN-N40)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/cc2531.pdf</description>
</package>
<package name="P-QFP48-7X7MM">
<description>&lt;b&gt;P-QFP48 7x7mm&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://focus.ti.com/lit/ds/symlink/bq78pl114.pdf"&gt; Datasheet &lt;/a&gt;</description>
</package>
<package name="ZCH(S-PBGA-N196)">
<description>&lt;b&gt;PLASTIC BALL GRID ARRAY&lt;/b&gt; ZCH (S-PBGA-N196)&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 36&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://focus.ti.com/lit/ds/symlink/tms320c5515.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="SWRA092B">
<description>&lt;b&gt;Compact Reach XtendTM Bluetooth®, 802.11b/g WLAN Chip Antenna&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/an/swra092b/swra092b.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="DCN-R-PDSO-G8">
<description>&lt;b&gt;DCN (R-PDSO-G8) PLASTIC SMALL-OUTLINE PACKAGE (DIE DOWN)&lt;/b&gt;&lt;p&gt;
Source: tps62120.pdf (www.ti.com)</description>
</package>
<package name="DRC-S-PVSON-N10">
<description>&lt;b&gt;DRK (S-PDSO-N10)&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. bq27010.pdf&lt;br&gt;
changed 2011-11-09</description>
</package>
<package name="DSC-S-PWSON-N10">
<description>&lt;b&gt;DSC (S-PWSON-N10)&lt;/b&gt;&lt;p&gt;
Source: http://www.ti.com/lit/ds/symlink/tps63060.pdf</description>
</package>
<package name="AAR">
<description>&lt;b&gt;DM385_AAR&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: DM385_AAR.bsdl</description>
</package>
<package name="RUG_(R-PQFP-N8)">
<description>RUG (S-PQFP-N8) PLASTIC QUAD FLATPACK&lt;p&gt;</description>
</package>
<package name="DCU_(R-PDSO-G8)">
<description>DCU (R-PDSO-G8) PLASTIC SMALL OUTLINE PACKAGE (DIE DOWN)&lt;/b&gt;&lt;p&gt;
Soure: &lt;a href="http://www.ti.com/lit/ds/symlink/ads7042.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
</packages>
<symbols>
<symbol name="320C5402">
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="A10" direction="in"/>
<pin name="HD7" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="A0" direction="in"/>
<pin name="HD6" direction="in"/>
<pin name="NC3" direction="nc"/>
<pin name="!HAS" direction="in"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="NC4" direction="nc"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="!HCS" direction="in"/>
<pin name="HR/!W" direction="in"/>
<pin name="READY" direction="in"/>
<pin name="!PS" direction="in"/>
<pin name="!DS" direction="in"/>
<pin name="!IS" direction="in"/>
<pin name="R/!W" direction="in"/>
<pin name="!MSTRB" direction="in"/>
<pin name="!IOSTRB" direction="in"/>
<pin name="!MSC" direction="in"/>
<pin name="XF" direction="in"/>
<pin name="!HOLDA" direction="in"/>
<pin name="!IAQ" direction="in"/>
<pin name="!HOLD" direction="in"/>
<pin name="!BIO" direction="in"/>
<pin name="MP/!MC" direction="in"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="NC5" direction="nc"/>
<pin name="NC6" direction="nc"/>
<pin name="NC7" direction="nc"/>
<pin name="NC8" direction="nc"/>
<pin name="HCNTL0" direction="in"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="BCLKR0" direction="in"/>
<pin name="BCLKR1" direction="in"/>
<pin name="BFSR0" direction="in"/>
<pin name="BFSR1" direction="in"/>
<pin name="HCNTL1" direction="in"/>
<pin name="BDR1" direction="in"/>
<pin name="BCLKX0" direction="in"/>
<pin name="BCLKX1" direction="in"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="!HINT" direction="in"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="BFSX0" direction="in"/>
<pin name="BFSX1" direction="in"/>
<pin name="HRDY" direction="in"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="HD0" direction="in"/>
<pin name="BDX0" direction="in"/>
<pin name="BDX1" direction="in"/>
<pin name="!IACK" direction="in"/>
<pin name="HBIL" direction="in"/>
<pin name="!NMI" direction="in"/>
<pin name="!INT0" direction="in"/>
<pin name="!INT1" direction="in"/>
<pin name="!INT2" direction="in"/>
<pin name="!INT3" direction="in"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="HD1" direction="in"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="NC9" direction="nc"/>
<pin name="NC10" direction="nc"/>
<pin name="NC11" direction="nc"/>
<pin name="NC12" direction="nc"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="CLKMD1" direction="in"/>
<pin name="CLKMD2" direction="in"/>
<pin name="CLKMD3" direction="in"/>
<pin name="NC13" direction="nc"/>
<pin name="HD2" direction="in"/>
<pin name="TOUT0" direction="in"/>
<pin name="EMU0" direction="in"/>
<pin name="EMU1/!OFF" direction="in"/>
<pin name="TDO" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="!TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NC14" direction="nc"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="HPIENA" direction="in"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="CLKOUT" direction="in"/>
<pin name="HD3" direction="in"/>
<pin name="X1" direction="in"/>
<pin name="X2/CLKIN" direction="in"/>
<pin name="!RS" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D8" direction="in"/>
<pin name="D9" direction="in"/>
<pin name="D10" direction="in"/>
<pin name="D11" direction="in"/>
<pin name="D12" direction="in"/>
<pin name="D13" direction="in"/>
<pin name="D14" direction="in"/>
<pin name="D15" direction="in"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="NC15" direction="nc"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="HD4" direction="in"/>
<pin name="HD5" direction="in"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="NC16" direction="nc"/>
<pin name="!HDS1" direction="in"/>
<pin name="!HDS2" direction="in"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="NC17" direction="nc"/>
<pin name="NC18" direction="nc"/>
<pin name="BDR0" direction="in"/>
</symbol>
<symbol name="TLV320AC">
<pin name="!PDN" direction="in"/>
<pin name="EARA" direction="out"/>
<pin name="EARB" direction="out"/>
<pin name="EARGS" direction="in"/>
<pin name="!MICMUTE" direction="in"/>
<pin name="DCLKR" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="FSR" direction="in"/>
<pin name="!EARMUTE" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="FSX" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="!TSX-DCLKX"/>
<pin name="!LINSEL" direction="in"/>
<pin name="VMID" direction="out"/>
<pin name="MICIN" direction="in"/>
<pin name="MICGS" direction="out"/>
<pin name="MICBIAS" direction="out"/>
</symbol>
<symbol name="VCCGND">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="AVCCGND">
<pin name="AVCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
</symbol>
<symbol name="DVCCGND">
<pin name="DVCC" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="320C54-B">
<pin name="A10" direction="hiz"/>
<pin name="HD7" direction="hiz"/>
<pin name="A11" direction="hiz"/>
<pin name="A1" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="A4" direction="hiz"/>
<pin name="A5" direction="hiz"/>
<pin name="A6" direction="hiz"/>
<pin name="A7" direction="hiz"/>
<pin name="A8" direction="hiz"/>
<pin name="A9" direction="hiz"/>
<pin name="A12" direction="hiz"/>
<pin name="A13" direction="hiz"/>
<pin name="A14" direction="hiz"/>
<pin name="A15" direction="hiz"/>
<pin name="A16" direction="hiz"/>
<pin name="A17" direction="hiz"/>
<pin name="A18" direction="hiz"/>
<pin name="A19" direction="hiz"/>
<pin name="A0" direction="hiz"/>
<pin name="HD6" direction="hiz"/>
<pin name="!HAS" direction="in"/>
<pin name="!HCS" direction="in"/>
<pin name="HR/!W" direction="in"/>
<pin name="READY" direction="in"/>
<pin name="!PS" direction="hiz"/>
<pin name="!DS" direction="hiz"/>
<pin name="!IS" direction="hiz"/>
<pin name="R/!W" direction="hiz"/>
<pin name="!MSTRB" direction="hiz"/>
<pin name="!IOSTRB" direction="hiz"/>
<pin name="!MSC" direction="hiz"/>
<pin name="XF" direction="hiz"/>
<pin name="!HOLDA" direction="hiz"/>
<pin name="!IAQ" direction="hiz"/>
<pin name="!HOLD" direction="in"/>
<pin name="!BIO" direction="in"/>
<pin name="MP/!MC" direction="in"/>
<pin name="HCNTL0" direction="in"/>
<pin name="BCLKR0" direction="hiz"/>
<pin name="BCLKR1" direction="hiz"/>
<pin name="BFSR0" direction="hiz"/>
<pin name="BFSR1" direction="hiz"/>
<pin name="HCNTL1" direction="in"/>
<pin name="BDR1" direction="in"/>
<pin name="BCLKX0" direction="hiz"/>
<pin name="BCLKX1" direction="hiz"/>
<pin name="!HINT" direction="hiz"/>
<pin name="BFSX0" direction="hiz"/>
<pin name="BFSX1" direction="hiz"/>
<pin name="HRDY" direction="hiz"/>
<pin name="HD0" direction="hiz"/>
<pin name="BDX0" direction="hiz"/>
<pin name="BDX1" direction="hiz"/>
<pin name="!IACK" direction="hiz"/>
<pin name="HBIL" direction="in"/>
<pin name="!NMI" direction="in"/>
<pin name="!INT0" direction="in"/>
<pin name="!INT1" direction="in"/>
<pin name="!INT2" direction="in"/>
<pin name="!INT3" direction="in"/>
<pin name="HD1" direction="hiz"/>
<pin name="CLKMD1" direction="in"/>
<pin name="CLKMD2" direction="in"/>
<pin name="CLKMD3" direction="in"/>
<pin name="HD2" direction="hiz"/>
<pin name="TOUT0" direction="hiz"/>
<pin name="EMU0" direction="hiz"/>
<pin name="EMU1/!OFF" direction="hiz"/>
<pin name="TDO" direction="hiz"/>
<pin name="TDI" direction="in"/>
<pin name="!TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="HPIENA" direction="in"/>
<pin name="CLKOUT" direction="hiz"/>
<pin name="HD3" direction="hiz"/>
<pin name="X1" direction="out"/>
<pin name="X2/CLKIN" direction="in"/>
<pin name="!RS" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
<pin name="HD4" direction="hiz"/>
<pin name="HD5" direction="hiz"/>
<pin name="!HDS1" direction="in"/>
<pin name="!HDS2" direction="in"/>
<pin name="BDR0" direction="in"/>
</symbol>
<symbol name="320PWR">
<pin name="VSS@1" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
</symbol>
<symbol name="L293E">
<pin name="1-2EN" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="2Y" direction="out"/>
<pin name="2A" direction="in"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="4A" direction="in"/>
<pin name="4Y" direction="out"/>
<pin name="GND3" direction="pwr"/>
<pin name="GND4" direction="pwr"/>
<pin name="3Y" direction="out"/>
<pin name="3A" direction="in"/>
<pin name="3-4EN" direction="in"/>
</symbol>
<symbol name="BQ2000">
<pin name="SNS" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="!LED" direction="out"/>
<pin name="BAT" direction="in"/>
<pin name="MOD" direction="out"/>
<pin name="VCC" direction="in"/>
<pin name="RC" direction="in"/>
<pin name="TS" direction="in"/>
</symbol>
<symbol name="BQ2054">
<pin name="VCOMP" direction="in"/>
<pin name="TS" direction="in"/>
<pin name="TPWM" direction="in"/>
<pin name="TM" direction="in"/>
<pin name="LED2/DSL" direction="hiz"/>
<pin name="SNS" direction="in"/>
<pin name="ICTL" direction="out" function="dot"/>
<pin name="VCC" direction="pwr"/>
<pin name="BAT" direction="in"/>
<pin name="ICOMP" direction="in"/>
<pin name="ITERM" direction="in"/>
<pin name="LED3" direction="hiz"/>
<pin name="LCOM" direction="out"/>
<pin name="VSS" direction="pwr"/>
<pin name="MOD" direction="out"/>
<pin name="LED1" direction="hiz"/>
</symbol>
<symbol name="BQ2058">
<pin name="CSL" direction="in"/>
<pin name="B1N" direction="in"/>
<pin name="B1P" direction="in"/>
<pin name="CHG" direction="hiz"/>
<pin name="DSG" direction="out"/>
<pin name="B2N2" direction="in"/>
<pin name="CTRL" direction="in"/>
<pin name="OVD" direction="in"/>
<pin name="VSS" direction="pwr"/>
<pin name="B2N" direction="in"/>
<pin name="B2N1" direction="in"/>
<pin name="CSH" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="OCD" direction="in"/>
<pin name="UVD" direction="in"/>
<pin name="VCC1" direction="pwr"/>
</symbol>
<symbol name="BQ2002">
<pin name="TM" direction="in"/>
<pin name="LED/" direction="oc"/>
<pin name="BAT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="TS" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="INH" direction="in"/>
<pin name="CC" direction="oc"/>
</symbol>
<symbol name="UC1843">
<pin name="COMP" direction="pas"/>
<pin name="SENSE" direction="in"/>
<pin name="RT/CT" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VFB" direction="in"/>
<pin name="VREF" direction="out"/>
<pin name="VC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="PWRGND" direction="pwr"/>
</symbol>
<symbol name="UC1526">
<pin name="+ERR" direction="in"/>
<pin name="-ERR" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="CSS" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="-SENSE" direction="in"/>
<pin name="+SENSE" direction="in"/>
<pin name="!SHDOWN" direction="out"/>
<pin name="RT" direction="pas"/>
<pin name="CT" direction="pas"/>
<pin name="RD" direction="pas"/>
<pin name="!SYNC" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="+VIN" direction="in"/>
<pin name="VREF" direction="out"/>
<pin name="VC" direction="in"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="UC1843-8">
<pin name="COMP" direction="pas"/>
<pin name="SENSE" direction="in"/>
<pin name="RT/CT" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="VFB" direction="in"/>
<pin name="VREF" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="TSL230">
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S3" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="DF1706">
<pin name="DIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="IIS" direction="in"/>
<pin name="IW0" direction="in"/>
<pin name="IW1" direction="in"/>
<pin name="XTI" direction="in"/>
<pin name="XTO" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="CLKO" direction="out"/>
<pin name="MODE" direction="in"/>
<pin name="MD/CKO" direction="in"/>
<pin name="MC/LRIP" direction="in"/>
<pin name="ML/RESV" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="!MUTE" direction="in"/>
<pin name="DEM" direction="in"/>
<pin name="SF0" direction="in"/>
<pin name="SF1" direction="in"/>
<pin name="OW0" direction="in"/>
<pin name="OW1" direction="in"/>
<pin name="OSS" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="DOR" direction="out"/>
<pin name="DOL" direction="out"/>
<pin name="WCKO" direction="out"/>
<pin name="BCKO" direction="out"/>
<pin name="SRO" direction="in"/>
<pin name="LRCIN" direction="in"/>
</symbol>
<symbol name="PCM2902">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="DGNDU" direction="pwr"/>
<pin name="HID0" direction="in"/>
<pin name="HID1" direction="in"/>
<pin name="HID2" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="VCCCI" direction="pwr"/>
<pin name="AGNDC" direction="pwr"/>
<pin name="VINL" direction="in"/>
<pin name="VINR" direction="in"/>
<pin name="VCOM" direction="pwr"/>
<pin name="VOUTR" direction="out"/>
<pin name="VOUTL" direction="out"/>
<pin name="VCCP1I" direction="in"/>
<pin name="AGNDP" direction="pwr"/>
<pin name="VCCP2I" direction="pwr"/>
<pin name="XTO" direction="out"/>
<pin name="XTI" direction="in"/>
<pin name="AGNDX" direction="pwr"/>
<pin name="VCCXI" direction="pwr"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDDI" direction="pwr"/>
<pin name="!SSPND" direction="out"/>
</symbol>
<symbol name="PCM2900">
<pin name="D+"/>
<pin name="D-"/>
<pin name="VBUS" direction="pwr"/>
<pin name="DGNDU" direction="pwr"/>
<pin name="HID0" direction="in"/>
<pin name="HID1" direction="in"/>
<pin name="HID2" direction="in"/>
<pin name="SEL0" direction="in"/>
<pin name="SEL1" direction="in"/>
<pin name="VCCCI" direction="pwr"/>
<pin name="AGNDC" direction="pwr"/>
<pin name="VINL" direction="in"/>
<pin name="VINR" direction="in"/>
<pin name="VCOM" direction="pwr"/>
<pin name="VOUTR" direction="out"/>
<pin name="VOUTL" direction="out"/>
<pin name="VCCP1I" direction="in"/>
<pin name="AGNDP" direction="pwr"/>
<pin name="VCCP2I" direction="pwr"/>
<pin name="XTO" direction="out"/>
<pin name="XTI" direction="in"/>
<pin name="AGNDX" direction="pwr"/>
<pin name="VCCXI" direction="pwr"/>
<pin name="TEST0" direction="in"/>
<pin name="TEST1" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDDI" direction="pwr"/>
<pin name="!SSPND" direction="out"/>
</symbol>
<symbol name="PLL1700">
<pin name="ML/SR0" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="XT2" direction="in"/>
<pin name="XT1" direction="in"/>
<pin name="DNGP" direction="pwr"/>
<pin name="VDDP" direction="pwr"/>
<pin name="RSV" direction="pas"/>
<pin name="MCKO" direction="out"/>
<pin name="!MCKO" direction="out"/>
<pin name="SCKO1" direction="out"/>
<pin name="SCKO4" direction="out"/>
<pin name="SCKO2" direction="out"/>
<pin name="GNDB" direction="pwr"/>
<pin name="VDDB" direction="pwr"/>
<pin name="SCKO3" direction="out"/>
<pin name="RST" direction="in"/>
<pin name="MD/FS0" direction="in"/>
<pin name="MD/FS1" direction="in"/>
</symbol>
<symbol name="TAS3001">
<pin name="CS2" direction="in"/>
<pin name="DVSS" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SDA"/>
<pin name="SCL"/>
<pin name="SDIN1" direction="in"/>
<pin name="SDIN2" direction="in"/>
<pin name="SDOUT" direction="out"/>
<pin name="MCLK" direction="in"/>
<pin name="LRCLK" direction="in"/>
<pin name="SCLK" direction="in"/>
<pin name="AVSS_PLL" direction="pwr"/>
<pin name="AVDD_PLL" direction="pwr"/>
<pin name="CAP_PLL" direction="in"/>
<pin name="RESERVED1" direction="in"/>
<pin name="POWDN" direction="in"/>
<pin name="NC1" direction="in"/>
<pin name="NC2" direction="in"/>
<pin name="!RES" direction="in"/>
<pin name="NC3" direction="in"/>
<pin name="NC4" direction="in"/>
<pin name="NC5" direction="in"/>
<pin name="LRCLKO" direction="out"/>
<pin name="SCLKO" direction="out"/>
<pin name="NC6" direction="in"/>
<pin name="NC7" direction="in"/>
<pin name="RESERVED2" direction="in"/>
<pin name="CS1" direction="in"/>
</symbol>
<symbol name="TAS3002">
<pin name="LINA" direction="in"/>
<pin name="VRFILT" direction="out"/>
<pin name="AVSS(REF)" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="!INPA" direction="out"/>
<pin name="!RES" direction="in"/>
<pin name="CS1" direction="in"/>
<pin name="PWR_DN" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="CAP_PLL" direction="in"/>
<pin name="CLKSEL" direction="in"/>
<pin name="MCLKO" direction="out"/>
<pin name="XTALI" direction="in"/>
<pin name="XTALO" direction="in"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="DVDD" direction="pwr"/>
<pin name="DVSS" direction="pwr"/>
<pin name="LRCLK/O"/>
<pin name="SCLK/O"/>
<pin name="IFM/!S" direction="in"/>
<pin name="SDIN1" direction="in"/>
<pin name="SDIN2" direction="in"/>
<pin name="SDOUT2" direction="out"/>
<pin name="SDOUT0" direction="out"/>
<pin name="SDOUT1" direction="out"/>
<pin name="GPI0" direction="in"/>
<pin name="GPI1" direction="in"/>
<pin name="GPI2" direction="in"/>
<pin name="GPI3" direction="in"/>
<pin name="GPI4" direction="in"/>
<pin name="GPI5" direction="in"/>
<pin name="NC1" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="NC2" direction="in"/>
<pin name="AUTOR" direction="out"/>
<pin name="VCOM" direction="pwr"/>
<pin name="AOUTL" direction="out"/>
<pin name="RINA" direction="in"/>
<pin name="RINB" direction="in"/>
<pin name="AINRP" direction="in"/>
<pin name="AINRM" direction="in"/>
<pin name="VREFP" direction="in"/>
<pin name="VREFM" direction="in"/>
<pin name="AINLM" direction="in"/>
<pin name="AINLP" direction="in"/>
<pin name="LINB" direction="in"/>
<pin name="ALLPASS" direction="in"/>
</symbol>
<symbol name="TMS320VC5402">
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="DVDD@0" direction="pwr"/>
<pin name="A10" direction="hiz"/>
<pin name="HD7" direction="hiz"/>
<pin name="A11" direction="hiz"/>
<pin name="A12" direction="hiz"/>
<pin name="A13" direction="hiz"/>
<pin name="A14" direction="hiz"/>
<pin name="A15" direction="hiz"/>
<pin name="NC@3" direction="nc"/>
<pin name="!HAS" direction="in"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="NC@4" direction="nc"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="!HCS" direction="in"/>
<pin name="HR/!W" direction="in"/>
<pin name="READY" direction="in"/>
<pin name="!PS" direction="hiz"/>
<pin name="!DS" direction="hiz"/>
<pin name="!IS" direction="hiz"/>
<pin name="R/!W" direction="hiz"/>
<pin name="!MSTRB" direction="hiz"/>
<pin name="!IOSTRB" direction="hiz"/>
<pin name="!MSC" direction="hiz"/>
<pin name="XF" direction="hiz"/>
<pin name="!HOLDA" direction="hiz"/>
<pin name="!IAQ" direction="hiz"/>
<pin name="!HOLD" direction="in"/>
<pin name="!BIO" direction="in"/>
<pin name="MP/!MC" direction="in"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="HCNTL0" direction="in"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="BCLKR0" direction="hiz"/>
<pin name="BCLKR1" direction="hiz"/>
<pin name="BFSR0" direction="hiz"/>
<pin name="BFSR1" direction="hiz"/>
<pin name="BDR0" direction="in"/>
<pin name="HCNTL1" direction="in"/>
<pin name="BDR1" direction="in"/>
<pin name="BCLKX0" direction="hiz"/>
<pin name="BCLKX1" direction="hiz"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="!HINT!/OUT1" direction="hiz"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="BFSX0" direction="hiz"/>
<pin name="BFSX1" direction="hiz"/>
<pin name="HRDY" direction="hiz"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="HD0" direction="hiz"/>
<pin name="BDX0" direction="hiz"/>
<pin name="BDX1" direction="hiz"/>
<pin name="!IACK" direction="hiz"/>
<pin name="HBIL" direction="in"/>
<pin name="!NMI" direction="in"/>
<pin name="!INT0" direction="in"/>
<pin name="!INT1" direction="in"/>
<pin name="!INT2" direction="in"/>
<pin name="!INT3" direction="in"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="HD1" direction="hiz"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="NC@9" direction="nc"/>
<pin name="NC@10" direction="nc"/>
<pin name="NC@11" direction="nc"/>
<pin name="NC@12" direction="nc"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="CLKMD1" direction="in"/>
<pin name="CLKMD2" direction="in"/>
<pin name="CLKMD3" direction="in"/>
<pin name="NC@13" direction="nc"/>
<pin name="HD2" direction="hiz"/>
<pin name="TOUT0" direction="hiz"/>
<pin name="EMU0" direction="hiz"/>
<pin name="EMU1" direction="hiz"/>
<pin name="TDO" direction="hiz"/>
<pin name="TDI" direction="in"/>
<pin name="!TRST" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="NC@14" direction="nc"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="HPIENA" direction="in"/>
<pin name="VSS@8" direction="nc"/>
<pin name="CLKOUT" direction="hiz"/>
<pin name="HD3" direction="hiz"/>
<pin name="X1" direction="out"/>
<pin name="X2" direction="in"/>
<pin name="!RS" direction="in"/>
<pin name="D0" direction="hiz"/>
<pin name="D1" direction="hiz"/>
<pin name="D2" direction="hiz"/>
<pin name="D3" direction="hiz"/>
<pin name="D4" direction="hiz"/>
<pin name="D5" direction="hiz"/>
<pin name="A16" direction="hiz"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="A17" direction="hiz"/>
<pin name="A18" direction="hiz"/>
<pin name="A19" direction="hiz"/>
<pin name="NC@15" direction="nc"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="D6" direction="hiz"/>
<pin name="D7" direction="hiz"/>
<pin name="D8" direction="hiz"/>
<pin name="D9" direction="hiz"/>
<pin name="D10" direction="hiz"/>
<pin name="D11" direction="hiz"/>
<pin name="D12" direction="hiz"/>
<pin name="HD4" direction="hiz"/>
<pin name="D13" direction="hiz"/>
<pin name="D14" direction="hiz"/>
<pin name="D15" direction="hiz"/>
<pin name="HD5" direction="hiz"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="NC@16" direction="nc"/>
<pin name="!HDS1" direction="in"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="!HDS2" direction="in"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="A0" direction="hiz"/>
<pin name="A1" direction="hiz"/>
<pin name="A2" direction="hiz"/>
<pin name="A3" direction="hiz"/>
<pin name="HD6" direction="hiz"/>
<pin name="A4" direction="hiz"/>
<pin name="A5" direction="hiz"/>
<pin name="A6" direction="hiz"/>
<pin name="A7" direction="hiz"/>
<pin name="A8" direction="hiz"/>
<pin name="A9" direction="hiz"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="NC@17" direction="nc"/>
<pin name="NC@18" direction="nc"/>
<pin name="VSS@12" direction="pwr"/>
</symbol>
<symbol name="TLC77XX">
<pin name="CONTROL" direction="in"/>
<pin name="!RESIN" direction="in"/>
<pin name="CT" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="!RESET" direction="out"/>
<pin name="RESET" direction="out"/>
<pin name="SENSE" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="MSP430F149">
<pin name="AVCC" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="DVCC" direction="pwr"/>
<pin name="DVSS" direction="pwr"/>
<pin name="P1.0"/>
<pin name="P1.1"/>
<pin name="P1.2"/>
<pin name="P1.3"/>
<pin name="P1.4"/>
<pin name="P1.5"/>
<pin name="P1.6"/>
<pin name="P1.7"/>
<pin name="P2.0"/>
<pin name="P2.1"/>
<pin name="P2.2"/>
<pin name="P2.3"/>
<pin name="P2.4"/>
<pin name="P2.5"/>
<pin name="P2.6"/>
<pin name="P2.7"/>
<pin name="P3.0"/>
<pin name="P3.1"/>
<pin name="P3.2"/>
<pin name="P3.3"/>
<pin name="P3.4"/>
<pin name="P3.5"/>
<pin name="P3.6"/>
<pin name="P3.7"/>
<pin name="P4.0"/>
<pin name="P4.1"/>
<pin name="P4.2"/>
<pin name="P4.3"/>
<pin name="P4.4"/>
<pin name="P4.5"/>
<pin name="P4.6"/>
<pin name="P4.7"/>
<pin name="P5.0"/>
<pin name="P5.1"/>
<pin name="P5.2"/>
<pin name="P5.3"/>
<pin name="P5.4"/>
<pin name="P5.5"/>
<pin name="P5.6"/>
<pin name="P5.7"/>
<pin name="P6.0"/>
<pin name="P6.1"/>
<pin name="P6.2"/>
<pin name="P6.3"/>
<pin name="P6.4"/>
<pin name="P6.5"/>
<pin name="P6.6"/>
<pin name="P6.7"/>
<pin name="!RTS!/NMI" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO/TDI"/>
<pin name="TMS" direction="in"/>
<pin name="VEREF+" direction="in"/>
<pin name="VREF+" direction="out"/>
<pin name="VREF-/VEREF-"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT/TCLK"/>
<pin name="XT2IN" direction="in"/>
<pin name="XT2OUT" direction="out"/>
</symbol>
<symbol name="OPAMP+-">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="THERMAL">
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="PCM3006">
<pin name="VINL" direction="in"/>
<pin name="VINR" direction="in"/>
<pin name="VOUTL" direction="out"/>
<pin name="VOUTR" direction="out"/>
<pin name="VREF1" direction="pas"/>
<pin name="VREF2" direction="pas"/>
<pin name="VCOM" direction="pwr"/>
<pin name="LRCIN" direction="in"/>
<pin name="BCKIN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="in"/>
<pin name="DEM0" direction="in"/>
<pin name="DEM1" direction="in"/>
<pin name="!PDAD" direction="in"/>
<pin name="!PDDA" direction="in"/>
<pin name="SYSCLOCK" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="GND@D" direction="pwr"/>
<pin name="GNDA" direction="pwr"/>
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VCC1@1" direction="pwr"/>
</symbol>
<symbol name="TPS75003">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="EN3" direction="in"/>
<pin name="SS1" direction="in"/>
<pin name="SS2" direction="in"/>
<pin name="SS3" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="IS1" direction="in"/>
<pin name="IS2" direction="in"/>
<pin name="SW1" direction="in"/>
<pin name="SW2" direction="in"/>
<pin name="FB1" direction="in"/>
<pin name="FB2" direction="in"/>
<pin name="FB3" direction="in"/>
<pin name="OUT3" direction="out"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DGND@4" direction="pwr"/>
<pin name="DGND@5" direction="pwr"/>
</symbol>
<symbol name="BQ24120">
<pin name="CELLS" direction="in"/>
<pin name="!PG" direction="out"/>
<pin name="SNS" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="STAT1" direction="out"/>
<pin name="ISET2"/>
<pin name="OUT1" direction="pas"/>
<pin name="PGND@2" direction="pas"/>
<pin name="BAT" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="ISET1"/>
<pin name="TS" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="PGND@1" direction="pas"/>
<pin name="TTC" direction="in"/>
<pin name="STAT2" direction="out"/>
<pin name="OUT2" direction="pas"/>
<pin name="VSS" direction="in"/>
<pin name="VTSB" direction="out"/>
<pin name="IN1" direction="in"/>
<pin name="EXP@1" direction="pas"/>
<pin name="EXP@2" direction="pas"/>
<pin name="EXP@3" direction="pas"/>
<pin name="EXP@4" direction="pas"/>
</symbol>
<symbol name="TL16C754B">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="GND"/>
<pin name="RXA"/>
<pin name="!RIA"/>
<pin name="!CDA"/>
<pin name="!DSRA"/>
<pin name="!CTSA"/>
<pin name="!DTRA"/>
<pin name="VCC"/>
<pin name="!RTSA"/>
<pin name="INTA"/>
<pin name="!CSA"/>
<pin name="TXA"/>
<pin name="!IOW"/>
<pin name="TXB"/>
<pin name="!CSB"/>
<pin name="INTB"/>
<pin name="!RTSB"/>
<pin name="GND@1"/>
<pin name="!DTRB"/>
<pin name="!CTSB"/>
<pin name="!DSRB"/>
<pin name="!CDB"/>
<pin name="!RIB"/>
<pin name="RXB"/>
<pin name="CLKSEL"/>
<pin name="NC"/>
<pin name="A0"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="XTAL1"/>
<pin name="XTAL2"/>
<pin name="RESET"/>
<pin name="!RXRDY"/>
<pin name="!TXRDY"/>
<pin name="GND@2"/>
<pin name="RXC"/>
<pin name="!RIC"/>
<pin name="!CDC"/>
<pin name="!DSRC"/>
<pin name="!CTSC"/>
<pin name="!DTRC"/>
<pin name="VCC@1"/>
<pin name="!RTSC"/>
<pin name="INTC"/>
<pin name="!CSC"/>
<pin name="TXC"/>
<pin name="!IOR"/>
<pin name="TXD"/>
<pin name="!CSD"/>
<pin name="INTD"/>
<pin name="!RTSD"/>
<pin name="GND@3"/>
<pin name="!DTRD"/>
<pin name="!CTSD"/>
<pin name="!DSRD"/>
<pin name="!CDD"/>
<pin name="!RID"/>
<pin name="RXD"/>
<pin name="VCC@2"/>
<pin name="INTESEL"/>
</symbol>
<symbol name="75ALS176">
<pin name="R" direction="out"/>
<pin name="D" direction="in"/>
<pin name="A"/>
<pin name="B" function="dot"/>
<pin name="DE" direction="in"/>
<pin name="!RE" direction="in"/>
</symbol>
<symbol name="TPS61070">
<pin name="SW" direction="in"/>
<pin name="VBAT" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="pas"/>
</symbol>
<symbol name="DDC232">
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="IN4" direction="in"/>
<pin name="IN5" direction="in"/>
<pin name="IN6" direction="in"/>
<pin name="IN7" direction="in"/>
<pin name="IN8" direction="in"/>
<pin name="IN9" direction="in"/>
<pin name="IN10" direction="in"/>
<pin name="IN11" direction="in"/>
<pin name="IN12" direction="in"/>
<pin name="IN13" direction="in"/>
<pin name="IN14" direction="in"/>
<pin name="IN15" direction="in"/>
<pin name="IN16" direction="in"/>
<pin name="IN17" direction="in"/>
<pin name="IN18" direction="in"/>
<pin name="IN19" direction="in"/>
<pin name="IN20" direction="in"/>
<pin name="IN21" direction="in"/>
<pin name="IN22" direction="in"/>
<pin name="IN23" direction="in"/>
<pin name="IN24" direction="in"/>
<pin name="IN25" direction="in"/>
<pin name="IN26" direction="in"/>
<pin name="IN27" direction="in"/>
<pin name="IN28" direction="in"/>
<pin name="IN29" direction="in"/>
<pin name="IN30" direction="in"/>
<pin name="IN31" direction="in"/>
<pin name="IN32" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="VREF" direction="pas"/>
<pin name="CLK" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="DIN_CFG" direction="in"/>
<pin name="CLK_CFG" direction="in"/>
<pin name="CONV" direction="in"/>
<pin name="!DVALID" direction="out"/>
<pin name="DCLK" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="VREF@1" direction="pas"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DGND@4" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AGND@5" direction="pwr"/>
<pin name="AGND@6" direction="pwr"/>
<pin name="AGND@7" direction="pwr"/>
<pin name="AGND@8" direction="pwr"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="QGND" direction="pwr"/>
</symbol>
<symbol name="TPS61200">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="PS" direction="in"/>
<pin name="UVLO" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VAUX"/>
<pin name="VOUT" direction="pas"/>
<pin name="L" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
<pin name="PP" direction="pwr"/>
<pin name="PP@1" direction="pwr"/>
<pin name="PP@2" direction="pwr"/>
</symbol>
<symbol name="MSP430FG4618">
<pin name="DVCC1" direction="pwr"/>
<pin name="P6_3/A3/OA1O"/>
<pin name="P6_4/A4/OA1I0"/>
<pin name="P6_5/A5/OA2O"/>
<pin name="P6_6/A6/DAC0/OA2I0"/>
<pin name="P6_7/A7/DAC1/SVSIN"/>
<pin name="VREF+" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="VEREF+/DAC0"/>
<pin name="VREF--/VEREF--" direction="in"/>
<pin name="P5_1/S0/A12/DAC1"/>
<pin name="P5_0/S1/A13/OA1I1"/>
<pin name="P10_7/S2/A14/OA2I1"/>
<pin name="P10_6/S3/A15"/>
<pin name="P10_5/S4"/>
<pin name="P10_4/S5"/>
<pin name="P10_3/S6"/>
<pin name="P10_2/S7"/>
<pin name="P10_1/S8"/>
<pin name="P10_0/S9"/>
<pin name="P9_7/S10"/>
<pin name="P9_6/S11"/>
<pin name="P9_5/S12"/>
<pin name="P9_4/S13"/>
<pin name="P9_3/S14"/>
<pin name="P9_2/S15"/>
<pin name="P9_1/S16"/>
<pin name="P9_0/S17"/>
<pin name="P8_7/S18"/>
<pin name="P8_6/S19"/>
<pin name="P8_5/S20"/>
<pin name="P8_4/S21"/>
<pin name="P8_3/S22"/>
<pin name="P8_2/S23"/>
<pin name="P8_1/S24"/>
<pin name="P8_0/S25"/>
<pin name="P7_7/S26"/>
<pin name="P7_6/S27"/>
<pin name="P7_5/S28"/>
<pin name="P7_4/S29"/>
<pin name="P7_3/UCA0CLK/S30"/>
<pin name="P7_2/UCA0SOMI/S31"/>
<pin name="P7_1/UCA0SIMO/S32"/>
<pin name="P7_0/UCA0STE/S33"/>
<pin name="P4_7/UCA0RXD/S34"/>
<pin name="P4_6/UCA0TXD/S35"/>
<pin name="P4_5/UCLK1/S36"/>
<pin name="P4_4/SOMI1/S37"/>
<pin name="P4_3/SIMO1/S38"/>
<pin name="P4_2/STE1/S39"/>
<pin name="COM0" direction="out"/>
<pin name="P5_2/COM1"/>
<pin name="P5_3/COM2"/>
<pin name="P5_4/COM3"/>
<pin name="P5_5/R03"/>
<pin name="P5_6/LCDREF/R13"/>
<pin name="P5_7/R23"/>
<pin name="LCDCAP/R33" direction="in"/>
<pin name="DVCC2" direction="pwr"/>
<pin name="DVSS2" direction="pwr"/>
<pin name="P4_1/URXD1"/>
<pin name="P4_0/UTXD1"/>
<pin name="P3_7/TB6"/>
<pin name="P3_6/TB5"/>
<pin name="P3_5/TB4"/>
<pin name="P3_4/TB3"/>
<pin name="P3_3/UCB0CLK"/>
<pin name="P3_2/UCB0SOMI/UCB0SCL"/>
<pin name="P3_1/UCB0SIMO/UCB0SDA"/>
<pin name="P3_0/UCB0STE"/>
<pin name="P2_7/ADC12CLK/DMAE0"/>
<pin name="P2_6/CAOUT"/>
<pin name="P2_5/UCA0RXD"/>
<pin name="P2_4/UCA0TXD"/>
<pin name="P2_3/TB2"/>
<pin name="P2_2/TB1"/>
<pin name="P2_1/TB0"/>
<pin name="P2_0/TA2"/>
<pin name="P1_7/CA1"/>
<pin name="P1_6/CA0"/>
<pin name="P1_5/TACLK/ACLK"/>
<pin name="P1_4/TBCLK/SMCLK"/>
<pin name="P1_3/TBOUTH/SVSOUT"/>
<pin name="P1_2/TA1"/>
<pin name="P1_1/TA0/MCLK"/>
<pin name="P1_0/TA0"/>
<pin name="XT2OUT" direction="out"/>
<pin name="XT2IN" direction="in"/>
<pin name="TDO/TDI"/>
<pin name="TDI/TCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="RST/NMI" direction="in"/>
<pin name="P6_0/A0/OA0I0"/>
<pin name="P6_1/A1/OA0O"/>
<pin name="P6_2/A2/OA0I1"/>
<pin name="AVSS" direction="pwr"/>
<pin name="DVSS1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="TPS3803">
<pin name="VDD" direction="pwr"/>
<pin name="SENSE" direction="in"/>
<pin name="!RESET" direction="out"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TLC7226">
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="!WR" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="REF" direction="in"/>
<pin name="VDD" direction="pwr"/>
</symbol>
<symbol name="SN65176">
<pin name="R" direction="in"/>
<pin name="!RE" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="D" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="VCC" direction="in"/>
</symbol>
<symbol name="OMAP3530">
<pin name="JTAG_TDI" direction="in"/>
<pin name="JTAG_TDO" direction="out"/>
<pin name="JTAG_TMS_TSMC" direction="in"/>
<pin name="JTAG_NTRST" direction="in"/>
<pin name="JTAG_TCK" direction="in"/>
<pin name="JTAG_RTCK" direction="pas"/>
<pin name="JTAG_EMU0" direction="pas"/>
<pin name="JTAG_EMU1" direction="pas"/>
<pin name="SYS_NRESPWRON" direction="pas"/>
<pin name="SYS_NRESWARM" direction="pas"/>
<pin name="SYS_OFF_MODE"/>
<pin name="SYS_BOOT6"/>
<pin name="SYS_BOOT5"/>
<pin name="SYS_BOOT4"/>
<pin name="SYS_BOOT3"/>
<pin name="SYS_BOOT2"/>
<pin name="SYS_BOOT1"/>
<pin name="SYS_BOOT0"/>
<pin name="I2C4_SCL"/>
<pin name="I2C4_SDA"/>
<pin name="SYS_XTALIN" direction="pas"/>
<pin name="SYS_XTALOUT" direction="pas"/>
<pin name="SYS_32K" direction="pas"/>
<pin name="SYS_CLKREQ"/>
<pin name="SYS_CLKOUT1"/>
<pin name="DSS_HSYNC"/>
<pin name="DSS_VSYNC"/>
<pin name="DSS_PCLK"/>
<pin name="DSS_DATA20"/>
<pin name="I2C1_SDA"/>
<pin name="I2C1_SCL"/>
<pin name="DSS_ACBIAS"/>
<pin name="DSS_DATA6"/>
<pin name="DSS_DATA7"/>
<pin name="DSS_DATA8"/>
<pin name="DSS_DATA9"/>
<pin name="DSS_DATA16"/>
<pin name="DSS_DATA17"/>
<pin name="DSS_DATA18"/>
<pin name="DSS_DATA19"/>
<pin name="DSS_DATA21"/>
<pin name="MCBSP1_FSX"/>
<pin name="HDQ_SIO"/>
<pin name="CAM_D8"/>
<pin name="CAM_D9"/>
<pin name="CAM_D7"/>
<pin name="CAM_D6"/>
<pin name="MMC1_CMD"/>
<pin name="MMC1_CLK"/>
<pin name="MMC1_DAT0"/>
<pin name="MMC1_DAT1"/>
<pin name="MMC1_DAT2"/>
<pin name="MMC1_DAT3"/>
<pin name="MMC1_DAT4"/>
<pin name="MMC1_DAT5"/>
<pin name="MMC1_DAT6"/>
<pin name="MMC1_DAT7"/>
<pin name="MCBSP2_DX"/>
<pin name="MCBSP2_CLKX"/>
<pin name="MCBSP2_FSX"/>
<pin name="MCBSP2_DR"/>
<pin name="MCBSP_CLKS"/>
<pin name="MCBSP1_DR"/>
<pin name="MCBSP1_DX"/>
<pin name="MCBSP1_CLKX"/>
<pin name="MCBSP1_CLKR"/>
<pin name="MCBSP1_FSR"/>
<pin name="HSUSB0_DIR"/>
<pin name="HSUSB0_NXT"/>
<pin name="HSUSB0_CLK"/>
<pin name="HSUSB0_STP"/>
<pin name="HSUSB0_DATA0"/>
<pin name="HSUSB0_DATA1"/>
<pin name="HSUSB0_DATA2"/>
<pin name="HSUSB0_DATA3"/>
<pin name="HSUSB0_DATA4"/>
<pin name="HSUSB0_DATA5"/>
<pin name="HSUSB0_DATA6"/>
<pin name="HSUSB0_DATA7"/>
<pin name="TV_VREF" direction="pas"/>
<pin name="TV_VFB2" direction="pas"/>
<pin name="TV_OUT2" direction="pas"/>
<pin name="TV_OUT1" direction="pas"/>
<pin name="TV_VFB1" direction="pas"/>
<pin name="DSS_DATA15"/>
<pin name="DSS_DATA14"/>
<pin name="DSS_DATA13"/>
<pin name="DSS_DATA12"/>
<pin name="DSS_DATA22"/>
<pin name="DSS_DATA23"/>
<pin name="DSS_DATA11"/>
<pin name="DSS_DATA10"/>
<pin name="UART2_TX"/>
<pin name="UART2_CTS"/>
<pin name="UART2_RTS"/>
<pin name="UART2_RX"/>
<pin name="DSS_DATA5"/>
<pin name="DSS_DATA4"/>
<pin name="DSS_DATA3"/>
<pin name="DSS_DATA2"/>
<pin name="DSS_DATA1"/>
<pin name="DSS_DATA0"/>
<pin name="GPIO_112"/>
<pin name="GPIO_113"/>
<pin name="GPIO_114"/>
<pin name="GPIO_115"/>
<pin name="CAM_D0"/>
<pin name="CAM_D1"/>
<pin name="SYS_NIRQ"/>
<pin name="SYS_CLKOUT2"/>
<pin name="I2C2_SCL"/>
<pin name="I2C2_SDA"/>
<pin name="I2C3_SCL"/>
<pin name="I2C3_SDA"/>
<pin name="ETK_D15"/>
<pin name="ETK_D14"/>
<pin name="ETK_D13"/>
<pin name="ETK_D12"/>
<pin name="ETK_D11"/>
<pin name="ETK_D7"/>
<pin name="ETK_D6"/>
<pin name="ETK_D3"/>
<pin name="ETK_D2"/>
<pin name="ETK_D1"/>
<pin name="ETK_D0"/>
<pin name="ETK_D4"/>
<pin name="ETK_D9"/>
<pin name="ETK_D8"/>
<pin name="ETK_CTL"/>
<pin name="ETK_CLK"/>
<pin name="ETK_D5"/>
<pin name="ETK_D10"/>
<pin name="UART1_RTS"/>
<pin name="UART1_TX"/>
<pin name="UART1_RX"/>
<pin name="UART1_CTS"/>
<pin name="MCBSP3_DX"/>
<pin name="MCBSP3_DR"/>
<pin name="MCBSP3_FSX"/>
<pin name="MCBSP3_CLKX"/>
<pin name="MMC2_CMD"/>
<pin name="MMC2_DAT0"/>
<pin name="MMC2_DAT1"/>
<pin name="MMC2_DAT2"/>
<pin name="MMC2_DAT3"/>
<pin name="MMC2_DAT4"/>
<pin name="MMC2_DAT5"/>
<pin name="MMC2_DAT6"/>
<pin name="MMC2_DAT7"/>
<pin name="MMC2_CLK"/>
<pin name="MCBSP4_CLKX"/>
<pin name="MCBSP4_DR"/>
<pin name="MCBSP4_DX"/>
<pin name="MCBSP4_FSX"/>
<pin name="MCSPI1_CS0"/>
<pin name="MCSPI1_CS1"/>
<pin name="MCSPI1_CS2"/>
<pin name="MCSPI1_CS3"/>
<pin name="MCSPI1_CLK"/>
<pin name="MCSPI1_SIMO"/>
<pin name="MCSPI1_SOMI"/>
<pin name="MCSPI2_CLK"/>
<pin name="MCSPI2_SIMO"/>
<pin name="MCSPI2_SOMI"/>
<pin name="MCSPI2_CS0"/>
<pin name="MCSPI2_CS1"/>
<pin name="GPMC_CLK"/>
<pin name="GPMC_D15"/>
<pin name="GPMC_D14"/>
<pin name="GPMC_D13"/>
<pin name="GPMC_D12"/>
<pin name="GPMC_D11"/>
<pin name="GPMC_D10"/>
<pin name="GPMC_D9"/>
<pin name="GPMC_D8"/>
<pin name="GPMC_D7"/>
<pin name="GPMC_D6"/>
<pin name="GPMC_D5"/>
<pin name="GPMC_D4"/>
<pin name="GPMC_D3"/>
<pin name="GPMC_D2"/>
<pin name="GPMC_D1"/>
<pin name="GPMC_D0"/>
<pin name="GPMC_NBE0_CLE"/>
<pin name="GPMC_NBE1"/>
<pin name="GPMC_A1"/>
<pin name="GPMC_A2"/>
<pin name="GPMC_A3"/>
<pin name="GPMC_A4"/>
<pin name="GPMC_A5"/>
<pin name="GPMC_A6"/>
<pin name="GPMC_A7"/>
<pin name="GPMC_A8"/>
<pin name="GPMC_A9"/>
<pin name="GPMC_A10"/>
<pin name="GPMC_NADV_ALE" direction="out"/>
<pin name="GPMC_NOE" direction="out"/>
<pin name="GPMC_NWE" direction="out"/>
<pin name="SYS_IPMCSWS" direction="pas"/>
<pin name="SYS_OPMCSWS" direction="pas"/>
<pin name="GPMC_NWP"/>
<pin name="GPMC_NCS0" direction="out"/>
<pin name="GPMC_NCS1"/>
<pin name="GPMC_NCS2"/>
<pin name="GPMC_NCS3"/>
<pin name="GPMC_NCS4"/>
<pin name="GPMC_NCS5"/>
<pin name="GPMC_NCS6"/>
<pin name="GPMC_NCS7"/>
<pin name="GPMC_WAIT0" direction="in"/>
<pin name="GPMC_WAIT1"/>
<pin name="GPMC_WAIT2"/>
<pin name="GPMC_WAIT3"/>
<pin name="CAM_VS"/>
<pin name="CAM_WEN"/>
<pin name="CAM_FLD"/>
<pin name="CAM_HS"/>
<pin name="CAM_D2"/>
<pin name="CAM_D3"/>
<pin name="CAM_D4"/>
<pin name="CAM_D5"/>
<pin name="CAM_D10"/>
<pin name="CAM_XCLKA"/>
<pin name="CAM_XCLKB"/>
<pin name="CAM_D11"/>
<pin name="CAM_PCLK"/>
<pin name="CAM_STROBE"/>
<pin name="UART3_CTS_RCTX"/>
<pin name="UART3_RTS_SD"/>
<pin name="UART3_RX_IRRX"/>
<pin name="UART3_TX_IRTX"/>
<pin name="SDRC_D0"/>
<pin name="SDRC_D1"/>
<pin name="SDRC_D2"/>
<pin name="SDRC_D3"/>
<pin name="SDRC_DM0" direction="out"/>
<pin name="SDRC_DQS0" direction="pas"/>
<pin name="SDRC_D4"/>
<pin name="SDRC_D5"/>
<pin name="SDRC_D6"/>
<pin name="SDRC_D7"/>
<pin name="SDRC_D16"/>
<pin name="SDRC_D17"/>
<pin name="SDRC_D18"/>
<pin name="SDRC_D19"/>
<pin name="SDRC_DM2" direction="out"/>
<pin name="SDRC_DQS2" direction="pas"/>
<pin name="SDRC_D20"/>
<pin name="SDRC_D21"/>
<pin name="SDRC_D22"/>
<pin name="SDRC_D23"/>
<pin name="SDRC_CLK" direction="pas"/>
<pin name="SDRC_NCLK" direction="pas"/>
<pin name="SDRC_D8"/>
<pin name="SDRC_D9"/>
<pin name="SDRC_D10"/>
<pin name="SDRC_D11"/>
<pin name="SDRC_DM1" direction="out"/>
<pin name="SDRC_DQS1" direction="pas"/>
<pin name="SDRC_D12"/>
<pin name="SDRC_D13"/>
<pin name="SDRC_D14"/>
<pin name="SDRC_D15"/>
<pin name="SDRC_D24"/>
<pin name="SDRC_D25"/>
<pin name="SDRC_D26"/>
<pin name="SDRC_D27"/>
<pin name="SDRC_DM3" direction="out"/>
<pin name="SDRC_DQS3" direction="pas"/>
<pin name="SDRC_D28"/>
<pin name="SDRC_D29"/>
<pin name="SDRC_D30"/>
<pin name="SDRC_D31"/>
<pin name="SDRC_BA0" direction="out"/>
<pin name="SDRC_BA1" direction="out"/>
<pin name="SDRC_NCS0" direction="out"/>
<pin name="SDRC_NCS1" direction="out"/>
<pin name="SDRC_NCAS" direction="out"/>
<pin name="SDRC_NRAS" direction="out"/>
<pin name="SDRC_NWE" direction="out"/>
<pin name="SDRC_CKE0" direction="out"/>
<pin name="SDRC_CKE1" direction="out"/>
<pin name="SDRC_A14" direction="out"/>
<pin name="SDRC_A13" direction="out"/>
<pin name="SDRC_A12" direction="out"/>
<pin name="SDRC_A11" direction="out"/>
<pin name="SDRC_A10" direction="out"/>
<pin name="SDRC_A9" direction="out"/>
<pin name="SDRC_A8" direction="out"/>
<pin name="SDRC_A7" direction="out"/>
<pin name="SDRC_A6" direction="out"/>
<pin name="SDRC_A5" direction="out"/>
<pin name="SDRC_A4" direction="out"/>
<pin name="SDRC_A3" direction="out"/>
<pin name="SDRC_A2" direction="out"/>
<pin name="SDRC_A1" direction="out"/>
<pin name="SDRC_A0" direction="out"/>
<pin name="BG_TESTOUT" direction="pas"/>
<pin name="VDD_MPU_IVA@0" direction="pwr"/>
<pin name="VDD_MPU_IVA@1" direction="pwr"/>
<pin name="VDD_MPU_IVA@2" direction="pwr"/>
<pin name="VDD_MPU_IVA@3" direction="pwr"/>
<pin name="VDD_MPU_IVA@4" direction="pwr"/>
<pin name="VDD_MPU_IVA@5" direction="pwr"/>
<pin name="VDD_MPU_IVA@6" direction="pwr"/>
<pin name="VDD_MPU_IVA@7" direction="pwr"/>
<pin name="VDD_MPU_IVA@8" direction="pwr"/>
<pin name="VDD_MPU_IVA@9" direction="pwr"/>
<pin name="VDD_MPU_IVA@10" direction="pwr"/>
<pin name="VDD_MPU_IVA@11" direction="pwr"/>
<pin name="VDD_MPU_IVA@12" direction="pwr"/>
<pin name="VDD_MPU_IVA@13" direction="pwr"/>
<pin name="VDD_MPU_IVA@14" direction="pwr"/>
<pin name="VDD_MPU_IVA@15" direction="pwr"/>
<pin name="VDD_MPU_IVA@16" direction="pwr"/>
<pin name="VDD_MPU_IVA@17" direction="pwr"/>
<pin name="VDD_MPU_IVA@18" direction="pwr"/>
<pin name="VDD_MPU_IVA@19" direction="pwr"/>
<pin name="VDD_MPU_IVA@20" direction="pwr"/>
<pin name="VDD_MPU_IVA@21" direction="pwr"/>
<pin name="VDD_MPU_IVA@22" direction="pwr"/>
<pin name="VDD_MPU_IVA@23" direction="pwr"/>
<pin name="VDD_MPU_IVA@24" direction="pwr"/>
<pin name="VDD_MPU_IVA@25" direction="pwr"/>
<pin name="VDD_MPU_IVA@26" direction="pwr"/>
<pin name="VDD_CORE@0" direction="pwr"/>
<pin name="VDD_CORE@1" direction="pwr"/>
<pin name="VDD_CORE@2" direction="pwr"/>
<pin name="VDD_CORE@3" direction="pwr"/>
<pin name="VDD_CORE@4" direction="pwr"/>
<pin name="VDD_CORE@5" direction="pwr"/>
<pin name="VDD_CORE@6" direction="pwr"/>
<pin name="VDD_CORE@7" direction="pwr"/>
<pin name="VDD_CORE@8" direction="pwr"/>
<pin name="VDD_CORE@9" direction="pwr"/>
<pin name="VDD_CORE@10" direction="pwr"/>
<pin name="VDD_CORE@11" direction="pwr"/>
<pin name="VDD_CORE@12" direction="pwr"/>
<pin name="VDD_CORE@13" direction="pwr"/>
<pin name="VDD_CORE@14" direction="pwr"/>
<pin name="VDD_CORE@15" direction="pwr"/>
<pin name="VDD_CORE@16" direction="pwr"/>
<pin name="VDD_CORE@17" direction="pwr"/>
<pin name="VDD_CORE@18" direction="pwr"/>
<pin name="VDD_CORE@19" direction="pwr"/>
<pin name="VDD_CORE@20" direction="pwr"/>
<pin name="VDD_CORE@21" direction="pwr"/>
<pin name="VDD_CORE@22" direction="pwr"/>
<pin name="VDD_CORE@23" direction="pwr"/>
<pin name="VDD_CORE@24" direction="pwr"/>
<pin name="VDD_CORE@25" direction="pwr"/>
<pin name="VDD_CORE@26" direction="pwr"/>
<pin name="VDD_CORE@27" direction="pwr"/>
<pin name="VDD_CORE@28" direction="pwr"/>
<pin name="VDD_CORE@29" direction="pwr"/>
<pin name="VDD_CORE@30" direction="pwr"/>
<pin name="VDD_CORE@31" direction="pwr"/>
<pin name="VDD_CORE@32" direction="pwr"/>
<pin name="VDD_CORE@33" direction="pwr"/>
<pin name="CAP_VDD_WKUP" direction="pwr"/>
<pin name="VDDA_DAC" direction="pwr"/>
<pin name="CAP_VDD_SRAM_MPU_IVA" direction="pwr"/>
<pin name="CAP_VDD_SRAM_CORE" direction="pwr"/>
<pin name="VDDS_DPLL_DLL" direction="pwr"/>
<pin name="VDDS_DPLL_PER" direction="pwr"/>
<pin name="VDDS_SRAM" direction="pwr"/>
<pin name="VDDS_WKUP_BG" direction="pwr"/>
<pin name="VDDS_MEM@0" direction="pwr"/>
<pin name="VDDS_MEM@1" direction="pwr"/>
<pin name="VDDS_MEM@2" direction="pwr"/>
<pin name="VDDS_MEM@3" direction="pwr"/>
<pin name="VDDS_MEM@4" direction="pwr"/>
<pin name="VDDS_MEM@5" direction="pwr"/>
<pin name="VDDS_MEM@6" direction="pwr"/>
<pin name="VDDS_MEM@7" direction="pwr"/>
<pin name="VDDS_MEM@8" direction="pwr"/>
<pin name="VDDS_MEM@9" direction="pwr"/>
<pin name="VDDS_MEM@10" direction="pwr"/>
<pin name="VDDS_MEM@11" direction="pwr"/>
<pin name="VDDS_MEM@12" direction="pwr"/>
<pin name="VDDS_MEM@13" direction="pwr"/>
<pin name="VDDS_MEM@14" direction="pwr"/>
<pin name="VDDS_MEM@15" direction="pwr"/>
<pin name="VDDS_MEM@16" direction="pwr"/>
<pin name="VDDS_MEM@17" direction="pwr"/>
<pin name="VDDS_MEM@18" direction="pwr"/>
<pin name="VDDS_MEM@19" direction="pwr"/>
<pin name="VDDS_MEM@20" direction="pwr"/>
<pin name="VDDS_MMC1" direction="pwr"/>
<pin name="VPP" direction="pas"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
<pin name="VSS@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="VSS@45" direction="pwr"/>
<pin name="VSS@46" direction="pwr"/>
<pin name="VSS@47" direction="pwr"/>
<pin name="VSS@48" direction="pwr"/>
<pin name="VSS@49" direction="pwr"/>
<pin name="VSS@50" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VSS@52" direction="pwr"/>
<pin name="VSS@53" direction="pwr"/>
<pin name="VSS@54" direction="pwr"/>
<pin name="VSS@55" direction="pwr"/>
<pin name="VSS@56" direction="pwr"/>
<pin name="VSS@57" direction="pwr"/>
<pin name="VSS@58" direction="pwr"/>
<pin name="VSS@59" direction="pwr"/>
<pin name="VSS@60" direction="pwr"/>
<pin name="VSS@61" direction="pwr"/>
<pin name="VSS@62" direction="pwr"/>
<pin name="VSS@63" direction="pwr"/>
<pin name="VSS@64" direction="pwr"/>
<pin name="VSS@65" direction="pwr"/>
<pin name="VSS@66" direction="pwr"/>
<pin name="VSS@67" direction="pwr"/>
<pin name="VSS@68" direction="pwr"/>
<pin name="VSS@69" direction="pwr"/>
<pin name="VSS@70" direction="pwr"/>
<pin name="POP_DDR_VDD_FT@0" direction="pwr"/>
<pin name="POP_DDR_VDD_FT@1" direction="pwr"/>
<pin name="POP_DDR_VDD_FT@2" direction="pwr"/>
<pin name="POP_DDR_VDD_FT@3" direction="pwr"/>
<pin name="POP_DDR_VDD_FT@4" direction="pwr"/>
<pin name="POP_FLASH_VPP_FT" direction="pas"/>
<pin name="POP_FLASH_VDD_FT@0" direction="pwr"/>
<pin name="POP_FLASH_VDD_FT@1" direction="pwr"/>
<pin name="POP_FLASH_VDD_FT@2" direction="pwr"/>
<pin name="POP_FLASH_VDD_FT@3" direction="pwr"/>
<pin name="POP_FLASH_VDD_FT@4" direction="pwr"/>
<pin name="POP_VSS_FT@0" direction="pwr"/>
<pin name="POP_VSS_FT@1" direction="pwr"/>
<pin name="POP_VSS_FT@2" direction="pwr"/>
<pin name="POP_VSS_FT@3" direction="pwr"/>
<pin name="POP_VSS_FT@4" direction="pwr"/>
<pin name="POP_VSS_FT@5" direction="pwr"/>
<pin name="POP_VSS_FT@6" direction="pwr"/>
<pin name="POP_VSS_FT@7" direction="pwr"/>
<pin name="POP_VSS_FT@8" direction="pwr"/>
<pin name="POP_VSS_FT@9" direction="pwr"/>
<pin name="VDDS@0" direction="pwr"/>
<pin name="VDDS@1" direction="pwr"/>
<pin name="VDDS@2" direction="pwr"/>
<pin name="VDDS@3" direction="pwr"/>
<pin name="VDDS@4" direction="pwr"/>
<pin name="VDDS@5" direction="pwr"/>
<pin name="VDDS@6" direction="pwr"/>
<pin name="VDDS@7" direction="pwr"/>
<pin name="VDDS@8" direction="pwr"/>
<pin name="VDDS@9" direction="pwr"/>
<pin name="VDDS@10" direction="pwr"/>
<pin name="VDDS@11" direction="pwr"/>
<pin name="VDDS@12" direction="pwr"/>
<pin name="VDDS@13" direction="pwr"/>
<pin name="VDDS@14" direction="pwr"/>
<pin name="VDDS@15" direction="pwr"/>
<pin name="VDDS@16" direction="pwr"/>
<pin name="VSSA_DAC" direction="pwr"/>
</symbol>
<symbol name="SPRM314">
<pin name="BG_TESTOUT"/>
<pin name="CAM_D0"/>
<pin name="CAM_D1"/>
<pin name="CAM_D2"/>
<pin name="CAM_D3"/>
<pin name="CAM_D4"/>
<pin name="CAM_D5"/>
<pin name="CAM_D6"/>
<pin name="CAM_D7"/>
<pin name="CAM_D8"/>
<pin name="CAM_D9"/>
<pin name="CAM_D10"/>
<pin name="CAM_D11"/>
<pin name="CAM_FLD"/>
<pin name="CAM_HS"/>
<pin name="CAM_PCLK"/>
<pin name="CAM_STROBE"/>
<pin name="CAM_VS"/>
<pin name="CAM_WEN"/>
<pin name="CAM_XCLKA"/>
<pin name="CAM_XCLKB"/>
<pin name="DSS_ACBIAS"/>
<pin name="DSS_DATA0"/>
<pin name="DSS_DATA1"/>
<pin name="DSS_DATA2"/>
<pin name="DSS_DATA3"/>
<pin name="DSS_DATA4"/>
<pin name="DSS_DATA5"/>
<pin name="DSS_DATA6"/>
<pin name="DSS_DATA7"/>
<pin name="DSS_DATA8"/>
<pin name="DSS_DATA9"/>
<pin name="DSS_DATA10"/>
<pin name="DSS_DATA11"/>
<pin name="DSS_DATA12"/>
<pin name="DSS_DATA13"/>
<pin name="DSS_DATA14"/>
<pin name="DSS_DATA15"/>
<pin name="DSS_DATA16"/>
<pin name="DSS_DATA17"/>
<pin name="DSS_DATA18"/>
<pin name="DSS_DATA19"/>
<pin name="DSS_DATA20"/>
<pin name="DSS_DATA21"/>
<pin name="DSS_DATA22"/>
<pin name="DSS_DATA23"/>
<pin name="DSS_HSYNC"/>
<pin name="DSS_PCLK"/>
<pin name="DSS_VSYNC"/>
<pin name="ETK_CLK"/>
<pin name="ETK_CTL"/>
<pin name="ETK_D0"/>
<pin name="ETK_D1"/>
<pin name="ETK_D2"/>
<pin name="ETK_D3"/>
<pin name="ETK_D4"/>
<pin name="ETK_D5"/>
<pin name="ETK_D6"/>
<pin name="ETK_D7"/>
<pin name="ETK_D8"/>
<pin name="ETK_D9"/>
<pin name="ETK_D10"/>
<pin name="ETK_D11"/>
<pin name="ETK_D12"/>
<pin name="ETK_D13"/>
<pin name="ETK_D14"/>
<pin name="ETK_D15"/>
<pin name="GPMC_A1"/>
<pin name="GPMC_A2"/>
<pin name="GPMC_A3"/>
<pin name="GPMC_A4"/>
<pin name="GPMC_A5"/>
<pin name="GPMC_A6"/>
<pin name="GPMC_A7"/>
<pin name="GPMC_A8"/>
<pin name="GPMC_A9"/>
<pin name="GPMC_A10"/>
<pin name="GPMC_CLK"/>
<pin name="GPMC_D0"/>
<pin name="GPMC_D1"/>
<pin name="GPMC_D2"/>
<pin name="GPMC_D3"/>
<pin name="GPMC_D4"/>
<pin name="GPMC_D5"/>
<pin name="GPMC_D6"/>
<pin name="GPMC_D7"/>
<pin name="GPMC_D8"/>
<pin name="GPMC_D9"/>
<pin name="GPMC_D10"/>
<pin name="GPMC_D11"/>
<pin name="GPMC_D12"/>
<pin name="GPMC_D13"/>
<pin name="GPMC_D14"/>
<pin name="GPMC_D15"/>
<pin name="GPMC_NADV_ALE" direction="out"/>
<pin name="GPMC_NBE0_CLE"/>
<pin name="GPMC_NBE1"/>
<pin name="GPMC_NCS0" direction="out"/>
<pin name="GPMC_NCS3"/>
<pin name="GPMC_NCS4"/>
<pin name="GPMC_NCS5"/>
<pin name="GPMC_NCS6"/>
<pin name="GPMC_NCS7"/>
<pin name="GPMC_NOE" direction="out"/>
<pin name="GPMC_NWE" direction="out"/>
<pin name="GPMC_NWP"/>
<pin name="GPMC_WAIT0" direction="in"/>
<pin name="GPMC_WAIT3"/>
<pin name="HDQ_SIO"/>
<pin name="HSUSB0_CLK"/>
<pin name="HSUSB0_DATA0"/>
<pin name="HSUSB0_DATA1"/>
<pin name="HSUSB0_DATA2"/>
<pin name="HSUSB0_DATA3"/>
<pin name="HSUSB0_DATA4"/>
<pin name="HSUSB0_DATA5"/>
<pin name="HSUSB0_DATA6"/>
<pin name="HSUSB0_DATA7"/>
<pin name="HSUSB0_DIR"/>
<pin name="HSUSB0_NXT"/>
<pin name="HSUSB0_STP"/>
<pin name="I2C1_SCL"/>
<pin name="I2C1_SDA"/>
<pin name="I2C2_SCL"/>
<pin name="I2C2_SDA"/>
<pin name="I2C3_SCL"/>
<pin name="I2C3_SDA"/>
<pin name="I2C4_SCL"/>
<pin name="I2C4_SDA"/>
<pin name="JTAG_EMU0" direction="pas"/>
<pin name="JTAG_EMU1" direction="pas"/>
<pin name="JTAG_NTRST" direction="in"/>
<pin name="JTAG_RTCK" direction="pas"/>
<pin name="JTAG_TCK" direction="in"/>
<pin name="JTAG_TDI" direction="in"/>
<pin name="JTAG_TDO" direction="out"/>
<pin name="JTAG_TMS_TSMC" direction="in"/>
<pin name="MCBSP1_CLKR"/>
<pin name="MCBSP1_CLKX"/>
<pin name="MCBSP1_DR"/>
<pin name="MCBSP1_DX"/>
<pin name="MCBSP1_FSR"/>
<pin name="MCBSP1_FSX"/>
<pin name="MCBSP2_CLKX"/>
<pin name="MCBSP2_DR"/>
<pin name="MCBSP2_DX"/>
<pin name="MCBSP2_FSX"/>
<pin name="MCBSP3_CLKX"/>
<pin name="MCBSP3_DR"/>
<pin name="MCBSP3_DX"/>
<pin name="MCBSP3_FSX"/>
<pin name="MCBSP_CLKS"/>
<pin name="MCSPI1_CLK"/>
<pin name="MCSPI1_CS0"/>
<pin name="MCSPI1_CS3"/>
<pin name="MCSPI1_SIMO"/>
<pin name="MCSPI1_SOMI"/>
<pin name="MCSPI2_CLK"/>
<pin name="MCSPI2_CS0"/>
<pin name="MCSPI2_CS1"/>
<pin name="MCSPI2_SIMO"/>
<pin name="MCSPI2_SOMI"/>
<pin name="MMC1_CLK"/>
<pin name="MMC1_CMD"/>
<pin name="MMC1_DAT0"/>
<pin name="MMC1_DAT1"/>
<pin name="MMC1_DAT2"/>
<pin name="MMC1_DAT3"/>
<pin name="MMC1_DAT4"/>
<pin name="MMC1_DAT5"/>
<pin name="MMC1_DAT6"/>
<pin name="MMC1_DAT7"/>
<pin name="MMC2_CLK"/>
<pin name="MMC2_CMD"/>
<pin name="MMC2_DAT0"/>
<pin name="MMC2_DAT1"/>
<pin name="MMC2_DAT2"/>
<pin name="MMC2_DAT3"/>
<pin name="MMC2_DAT4"/>
<pin name="MMC2_DAT5"/>
<pin name="MMC2_DAT6"/>
<pin name="MMC2_DAT7"/>
<pin name="SDRC_A0" direction="out"/>
<pin name="SDRC_A1" direction="out"/>
<pin name="SDRC_A2" direction="out"/>
<pin name="SDRC_A3" direction="out"/>
<pin name="SDRC_A4" direction="out"/>
<pin name="SDRC_A5" direction="out"/>
<pin name="SDRC_A6" direction="out"/>
<pin name="SDRC_A7" direction="out"/>
<pin name="SDRC_A8" direction="out"/>
<pin name="SDRC_A9" direction="out"/>
<pin name="SDRC_A10" direction="out"/>
<pin name="SDRC_A11" direction="out"/>
<pin name="SDRC_A12" direction="out"/>
<pin name="SDRC_A13" direction="out"/>
<pin name="SDRC_A14" direction="out"/>
<pin name="SDRC_BA0" direction="out"/>
<pin name="SDRC_BA1" direction="out"/>
<pin name="SDRC_CKE0" direction="out"/>
<pin name="SDRC_CKE1" direction="out"/>
<pin name="SDRC_CLK" direction="pas"/>
<pin name="SDRC_D0"/>
<pin name="SDRC_D1"/>
<pin name="SDRC_D2"/>
<pin name="SDRC_D3"/>
<pin name="SDRC_D4"/>
<pin name="SDRC_D5"/>
<pin name="SDRC_D6"/>
<pin name="SDRC_D7"/>
<pin name="SDRC_D8"/>
<pin name="SDRC_D9"/>
<pin name="SDRC_D10"/>
<pin name="SDRC_D11"/>
<pin name="SDRC_D12"/>
<pin name="SDRC_D13"/>
<pin name="SDRC_D14"/>
<pin name="SDRC_D15"/>
<pin name="SDRC_D16"/>
<pin name="SDRC_D17"/>
<pin name="SDRC_D18"/>
<pin name="SDRC_D19"/>
<pin name="SDRC_D20"/>
<pin name="SDRC_D21"/>
<pin name="SDRC_D22"/>
<pin name="SDRC_D23"/>
<pin name="SDRC_D24"/>
<pin name="SDRC_D25"/>
<pin name="SDRC_D26"/>
<pin name="SDRC_D27"/>
<pin name="SDRC_D28"/>
<pin name="SDRC_D29"/>
<pin name="SDRC_D30"/>
<pin name="SDRC_D31"/>
<pin name="SDRC_DM0" direction="out"/>
<pin name="SDRC_DM1" direction="out"/>
<pin name="SDRC_DM2" direction="out"/>
<pin name="SDRC_DM3" direction="out"/>
<pin name="SDRC_DQS0" direction="pas"/>
<pin name="SDRC_DQS1" direction="pas"/>
<pin name="SDRC_DQS2" direction="pas"/>
<pin name="SDRC_DQS3" direction="pas"/>
<pin name="SDRC_NCAS" direction="out"/>
<pin name="SDRC_NCLK" direction="pas"/>
<pin name="SDRC_NCS0" direction="out"/>
<pin name="SDRC_NCS1" direction="out"/>
<pin name="SDRC_NRAS" direction="out"/>
<pin name="SDRC_NWE" direction="out"/>
<pin name="SYS_32K" direction="pas"/>
<pin name="SYS_BOOT0"/>
<pin name="SYS_BOOT1"/>
<pin name="SYS_BOOT2"/>
<pin name="SYS_BOOT3"/>
<pin name="SYS_BOOT4"/>
<pin name="SYS_BOOT5"/>
<pin name="SYS_BOOT6"/>
<pin name="SYS_CLKOUT1"/>
<pin name="SYS_CLKOUT2"/>
<pin name="SYS_CLKREQ"/>
<pin name="SYS_IPMCSWS" direction="pas"/>
<pin name="SYS_NIRQ"/>
<pin name="SYS_NRESPWRON" direction="pas"/>
<pin name="SYS_NRESWARM" direction="pas"/>
<pin name="SYS_OFF_MODE"/>
<pin name="SYS_OPMCSWS" direction="pas"/>
<pin name="SYS_XTALIN" direction="pas"/>
<pin name="SYS_XTALOUT" direction="pas"/>
<pin name="TV_OUT1" direction="pas"/>
<pin name="TV_OUT2" direction="pas"/>
<pin name="TV_VFB1" direction="pas"/>
<pin name="TV_VFB2" direction="pas"/>
<pin name="TV_VREF" direction="pas"/>
<pin name="UART1_CTS"/>
<pin name="UART1_RTS"/>
<pin name="UART1_RX"/>
<pin name="UART1_TX"/>
<pin name="UART3_CTS_RCTX"/>
<pin name="UART3_RTS_SD"/>
<pin name="UART3_RX_IRRX"/>
<pin name="UART3_TX_IRTX"/>
<pin name="VDD_MPU_IVA@0" direction="pwr"/>
<pin name="VDD_MPU_IVA@1" direction="pwr"/>
<pin name="VDD_MPU_IVA@2" direction="pwr"/>
<pin name="VDD_MPU_IVA@3" direction="pwr"/>
<pin name="VDD_MPU_IVA@4" direction="pwr"/>
<pin name="VDD_MPU_IVA@5" direction="pwr"/>
<pin name="VDD_MPU_IVA@6" direction="pwr"/>
<pin name="VDD_MPU_IVA@7" direction="pwr"/>
<pin name="VDD_MPU_IVA@8" direction="pwr"/>
<pin name="VDD_MPU_IVA@9" direction="pwr"/>
<pin name="VDD_MPU_IVA@10" direction="pwr"/>
<pin name="VDD_MPU_IVA@11" direction="pwr"/>
<pin name="VDD_MPU_IVA@12" direction="pwr"/>
<pin name="VDD_MPU_IVA@13" direction="pwr"/>
<pin name="VDD_MPU_IVA@14" direction="pwr"/>
<pin name="VDD_MPU_IVA@15" direction="pwr"/>
<pin name="VDD_MPU_IVA@16" direction="pwr"/>
<pin name="VDD_MPU_IVA@17" direction="pwr"/>
<pin name="VDD_MPU_IVA@18" direction="pwr"/>
<pin name="VDD_MPU_IVA@19" direction="pwr"/>
<pin name="VDD_MPU_IVA@20" direction="pwr"/>
<pin name="VDD_MPU_IVA@21" direction="pwr"/>
<pin name="VDD_MPU_IVA@22" direction="pwr"/>
<pin name="VDD_MPU_IVA@23" direction="pwr"/>
<pin name="VDD_MPU_IVA@24" direction="pwr"/>
<pin name="VDD_MPU_IVA@25" direction="pwr"/>
<pin name="VDD_MPU_IVA@26" direction="pwr"/>
<pin name="VDD_CORE@0" direction="pwr"/>
<pin name="VDD_CORE@1" direction="pwr"/>
<pin name="VDD_CORE@2" direction="pwr"/>
<pin name="VDD_CORE@3" direction="pwr"/>
<pin name="VDD_CORE@4" direction="pwr"/>
<pin name="VDD_CORE@5" direction="pwr"/>
<pin name="VDD_CORE@6" direction="pwr"/>
<pin name="VDD_CORE@7" direction="pwr"/>
<pin name="VDD_CORE@8" direction="pwr"/>
<pin name="VDD_CORE@9" direction="pwr"/>
<pin name="VDD_CORE@10" direction="pwr"/>
<pin name="VDD_CORE@11" direction="pwr"/>
<pin name="VDD_CORE@12" direction="pwr"/>
<pin name="VDD_CORE@13" direction="pwr"/>
<pin name="VDD_CORE@14" direction="pwr"/>
<pin name="VDD_CORE@15" direction="pwr"/>
<pin name="VDD_CORE@16" direction="pwr"/>
<pin name="VDD_CORE@17" direction="pwr"/>
<pin name="VDD_CORE@18" direction="pwr"/>
<pin name="VDD_CORE@19" direction="pwr"/>
<pin name="VDD_CORE@20" direction="pwr"/>
<pin name="VDD_CORE@21" direction="pwr"/>
<pin name="CAP_VDD_SRAM_CORE" direction="pwr"/>
<pin name="CAP_VDD_SRAM_MPU_IVA" direction="pwr"/>
<pin name="CAP_VDD_WKUP" direction="pwr"/>
<pin name="VDDA_DAC" direction="pwr"/>
<pin name="VDDS@0" direction="pwr"/>
<pin name="VDDS@1" direction="pwr"/>
<pin name="VDDS@2" direction="pwr"/>
<pin name="VDDS@3" direction="pwr"/>
<pin name="VDDS@4" direction="pwr"/>
<pin name="VDDS@5" direction="pwr"/>
<pin name="VDDS@6" direction="pwr"/>
<pin name="VDDS@7" direction="pwr"/>
<pin name="VDDS@8" direction="pwr"/>
<pin name="VDDS@9" direction="pwr"/>
<pin name="VDDS@10" direction="pwr"/>
<pin name="VDDS@11" direction="pwr"/>
<pin name="VDDS@12" direction="pwr"/>
<pin name="VDDS_DPLL_DLL" direction="pwr"/>
<pin name="VDDS_DPLL_PER" direction="pwr"/>
<pin name="VDDS_MEM@0" direction="pwr"/>
<pin name="VDDS_MEM@1" direction="pwr"/>
<pin name="VDDS_MEM@2" direction="pwr"/>
<pin name="VDDS_MEM@3" direction="pwr"/>
<pin name="VDDS_MEM@4" direction="pwr"/>
<pin name="VDDS_MEM@5" direction="pwr"/>
<pin name="VDDS_MEM@6" direction="pwr"/>
<pin name="VDDS_MEM@7" direction="pwr"/>
<pin name="VDDS_MEM@8" direction="pwr"/>
<pin name="VDDS_MEM@9" direction="pwr"/>
<pin name="VDDS_MEM@10" direction="pwr"/>
<pin name="VDDS_MEM@11" direction="pwr"/>
<pin name="VDDS_MMC1" direction="pwr"/>
<pin name="VDDS_SRAM" direction="pwr"/>
<pin name="VDDS_WKUP_BG" direction="pwr"/>
<pin name="VPP" direction="pas"/>
<pin name="VSS@0" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
<pin name="VSS@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="VSS@45" direction="pwr"/>
<pin name="VSS@46" direction="pwr"/>
<pin name="VSS@47" direction="pwr"/>
<pin name="VSS@48" direction="pwr"/>
<pin name="VSS@49" direction="pwr"/>
<pin name="VSS@50" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VSS@52" direction="pwr"/>
<pin name="VSS@53" direction="pwr"/>
<pin name="VSS@54" direction="pwr"/>
<pin name="VSS@55" direction="pwr"/>
<pin name="VSS@56" direction="pwr"/>
<pin name="VSS@57" direction="pwr"/>
<pin name="VSSA_DAC" direction="pwr"/>
</symbol>
<symbol name="TPS65023">
<pin name="DEFDCDC3" direction="in"/>
<pin name="VDCDC3" direction="in"/>
<pin name="PGND3" direction="in"/>
<pin name="L3" direction="pas"/>
<pin name="VINDCDC3" direction="in"/>
<pin name="VINDCDC1" direction="in"/>
<pin name="L1" direction="pas"/>
<pin name="PGND1" direction="in"/>
<pin name="VDCDC1" direction="in"/>
<pin name="DEFDCDC1" direction="in"/>
<pin name="!HOT_RESET" direction="in"/>
<pin name="DEFLDO1" direction="in"/>
<pin name="DEFLDO2" direction="in"/>
<pin name="VSYSIN" direction="in"/>
<pin name="VBACKUP" direction="in"/>
<pin name="VRTC" direction="out"/>
<pin name="AGND2" direction="in"/>
<pin name="VLDO2" direction="out"/>
<pin name="VINLDO" direction="in"/>
<pin name="VLDO1" direction="out"/>
<pin name="!LOWBAT" direction="oc"/>
<pin name="LDO_EN" direction="in"/>
<pin name="DCDC3_EN" direction="in"/>
<pin name="DCDC2_EN" direction="in"/>
<pin name="DCDC1_EN" direction="in"/>
<pin name="TRESPWRON" direction="in"/>
<pin name="!RESPWRON" direction="oc"/>
<pin name="!INT" direction="oc"/>
<pin name="SDAT"/>
<pin name="SCLK" direction="in"/>
<pin name="!PWRFAIL" direction="oc"/>
<pin name="DEFDCDC2" direction="in"/>
<pin name="VDCDC2" direction="in"/>
<pin name="PGND2" direction="in"/>
<pin name="L2" direction="pas"/>
<pin name="VINDCDC2" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="PWRFAIL_SNS" direction="in"/>
<pin name="LOWBAT_SNS" direction="in"/>
<pin name="AGND1" direction="in"/>
</symbol>
<symbol name="TPS65020">
<pin name="DEFDCDC3" direction="in"/>
<pin name="VDCDC3" direction="in"/>
<pin name="PGND3" direction="in"/>
<pin name="L3" direction="pas"/>
<pin name="VINDCDC3" direction="in"/>
<pin name="VINDCDC1" direction="in"/>
<pin name="L1" direction="pas"/>
<pin name="PGND1" direction="in"/>
<pin name="VDCDC1" direction="in"/>
<pin name="DEFDCDC1" direction="in"/>
<pin name="!HOT_RESET" direction="in"/>
<pin name="PB_IN" direction="in"/>
<pin name="PB_OUT" direction="in"/>
<pin name="VSYSIN" direction="in"/>
<pin name="VBACKUP" direction="in"/>
<pin name="VRTC" direction="out"/>
<pin name="AGND2" direction="in"/>
<pin name="VLDO2" direction="out"/>
<pin name="VINLDO" direction="in"/>
<pin name="VLDO1" direction="out"/>
<pin name="!LOWBAT" direction="oc"/>
<pin name="LDO_EN" direction="in"/>
<pin name="DCDC3_EN" direction="in"/>
<pin name="DCDC2_EN" direction="in"/>
<pin name="DCDC1_EN" direction="in"/>
<pin name="TRESPWRON" direction="in"/>
<pin name="!RESPWRON" direction="oc"/>
<pin name="!INT" direction="oc"/>
<pin name="SDAT"/>
<pin name="SCLK" direction="in"/>
<pin name="!PWRFAIL" direction="oc"/>
<pin name="DEFDCDC2" direction="in"/>
<pin name="VDCDC2" direction="in"/>
<pin name="PGND2" direction="in"/>
<pin name="L2" direction="pas"/>
<pin name="VINDCDC2" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="PWRFAIL_SNS" direction="in"/>
<pin name="LOWBAT_SNS" direction="in"/>
<pin name="AGND1" direction="in"/>
</symbol>
<symbol name="EXP-16">
<pin name="EXP16@1" direction="in"/>
<pin name="EXP16@2" direction="in"/>
<pin name="EXP16@3" direction="in"/>
<pin name="EXP16@4" direction="in"/>
<pin name="EXP16@5" direction="in"/>
<pin name="EXP16@6" direction="in"/>
<pin name="EXP16@7" direction="in"/>
<pin name="EXP16@8" direction="in"/>
<pin name="EXP16@9" direction="in"/>
<pin name="EXP16@10" direction="in"/>
<pin name="EXP16@11" direction="in"/>
<pin name="EXP16@12" direction="in"/>
<pin name="EXP16@13" direction="in"/>
<pin name="EXP16@14" direction="in"/>
<pin name="EXP16@15" direction="in"/>
<pin name="EXP16@16" direction="in"/>
</symbol>
<symbol name="EXP17">
<pin name="EXP16@1" direction="in"/>
<pin name="EXP16@2" direction="in"/>
<pin name="EXP16@3" direction="in"/>
<pin name="EXP16@4" direction="in"/>
<pin name="EXP16@5" direction="in"/>
<pin name="EXP16@6" direction="in"/>
<pin name="EXP16@7" direction="in"/>
<pin name="EXP16@8" direction="in"/>
<pin name="EXP16@9" direction="in"/>
<pin name="EXP16@10" direction="in"/>
<pin name="EXP16@11" direction="in"/>
<pin name="EXP16@12" direction="in"/>
<pin name="EXP16@13" direction="in"/>
<pin name="EXP16@14" direction="in"/>
<pin name="EXP16@15" direction="in"/>
<pin name="EXP16@16" direction="in"/>
<pin name="EXP" direction="in"/>
</symbol>
<symbol name="BQ24120-1">
<pin name="OUT@1" direction="out"/>
<pin name="STAT1" direction="out"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="!PG" direction="out"/>
<pin name="VCC" direction="in"/>
<pin name="TTC" direction="pas"/>
<pin name="ISET1"/>
<pin name="ISET2"/>
<pin name="VSS" direction="pwr"/>
<pin name="VTSB" direction="out"/>
<pin name="TS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="BAT" direction="in"/>
<pin name="SNS" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="PGND@1" direction="in"/>
<pin name="PGND@2" direction="in"/>
<pin name="STAT2" direction="out"/>
<pin name="OUT@2" direction="in"/>
</symbol>
<symbol name="EXP">
<pin name="1" direction="in"/>
<pin name="2" direction="in"/>
<pin name="3" direction="in"/>
<pin name="4" direction="in"/>
<pin name="5" direction="in"/>
<pin name="6" direction="in"/>
<pin name="7" direction="in"/>
<pin name="8" direction="in"/>
<pin name="9" direction="in"/>
<pin name="10" direction="in"/>
<pin name="11" direction="in"/>
<pin name="12" direction="in"/>
<pin name="13" direction="in"/>
</symbol>
<symbol name="BQ24123">
<pin name="OUT@1" direction="out"/>
<pin name="STAT1" direction="out"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="!PG" direction="out"/>
<pin name="VCC" direction="in"/>
<pin name="TTC" direction="pas"/>
<pin name="ISET1"/>
<pin name="ISET2"/>
<pin name="VSS" direction="pwr"/>
<pin name="VTSB" direction="out"/>
<pin name="TS" direction="in"/>
<pin name="CELLS" direction="in"/>
<pin name="BAT" direction="in"/>
<pin name="SNS" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="PGND@1" direction="in"/>
<pin name="PGND@2" direction="in"/>
<pin name="STAT2" direction="out"/>
<pin name="OUT@2" direction="in"/>
</symbol>
<symbol name="BQ24125">
<pin name="OUT@1" direction="out"/>
<pin name="STAT1" direction="out"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="!PG" direction="out"/>
<pin name="VCC" direction="in"/>
<pin name="TTC" direction="pas"/>
<pin name="ISET1"/>
<pin name="ISET2"/>
<pin name="VSS" direction="pwr"/>
<pin name="VTSB" direction="out"/>
<pin name="TS" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="BAT" direction="in"/>
<pin name="SNS" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="PGND@1" direction="in"/>
<pin name="PGND@2" direction="in"/>
<pin name="STAT2" direction="out"/>
<pin name="OUT@2" direction="in"/>
</symbol>
<symbol name="BQ27500">
<pin name="BAT_LOW" direction="out"/>
<pin name="BI/TOUT"/>
<pin name="TS" direction="in"/>
<pin name="BAT" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="SRP" direction="in"/>
<pin name="SRN" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="!BAT_GD" direction="out"/>
</symbol>
<symbol name="BQ27501">
<pin name="BAT_LOW" direction="out"/>
<pin name="BI/TOUT"/>
<pin name="TS" direction="in"/>
<pin name="BAT" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="SRP" direction="in"/>
<pin name="SRN" direction="in"/>
<pin name="RID" direction="in"/>
<pin name="SDA"/>
<pin name="SCL" direction="in"/>
<pin name="!BAT_GD" direction="out"/>
</symbol>
<symbol name="PWPD9">
<pin name="PWPD@1" direction="pwr"/>
<pin name="PWPD@2" direction="pwr"/>
<pin name="PWPD@3" direction="pwr"/>
<pin name="PWPD@4" direction="pwr"/>
<pin name="PWPD@5" direction="pwr"/>
<pin name="PWPD@6" direction="pwr"/>
<pin name="PWPD@7" direction="pwr"/>
<pin name="PWPD@8" direction="pwr"/>
<pin name="PWPD@9" direction="pwr"/>
</symbol>
<symbol name="ISO7240">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND1@1" direction="pwr"/>
<pin name="GND1@2" direction="pwr"/>
<pin name="GND2@1" direction="pwr"/>
<pin name="GND2@2" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="EN" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="ISO7241">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND1@1" direction="pwr"/>
<pin name="GND1@2" direction="pwr"/>
<pin name="GND2@1" direction="pwr"/>
<pin name="GND2@2" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="ISO7242">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND1@1" direction="pwr"/>
<pin name="GND1@2" direction="pwr"/>
<pin name="GND2@1" direction="pwr"/>
<pin name="GND2@2" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="INC" direction="in"/>
<pin name="IND" direction="in"/>
<pin name="EN1" direction="in"/>
<pin name="EN2" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
<pin name="OUTC" direction="out"/>
<pin name="OUTD" direction="out"/>
</symbol>
<symbol name="ISO7220">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="ISO7221">
<pin name="VCC1" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="GND1" direction="pwr"/>
<pin name="GND2" direction="pwr"/>
<pin name="INA" direction="in"/>
<pin name="INB" direction="in"/>
<pin name="OUTA" direction="out"/>
<pin name="OUTB" direction="out"/>
</symbol>
<symbol name="TPS770XX">
<pin name="IN" direction="in"/>
<pin name="!EN" direction="in"/>
<pin name="NC/FB" direction="pas"/>
<pin name="OUT" direction="pas"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="MSP430XW42X">
<pin name="DVCC" direction="pwr"/>
<pin name="P6_3/SIFCH3/SIFCAOUT"/>
<pin name="P6_4/SIFCI0"/>
<pin name="P6_5/SIFCI1"/>
<pin name="P6_6/SIFCI2/SIFDACOUT"/>
<pin name="P6_7/SIFCI3/SVSIN"/>
<pin name="SIFCI" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="SIFVSS" direction="pas"/>
<pin name="SIFCOM" direction="out"/>
<pin name="P5_1/S0"/>
<pin name="P5_0/S1"/>
<pin name="P4_7/S2"/>
<pin name="P4_6/S3"/>
<pin name="P4_5/S4"/>
<pin name="P4_4/S5"/>
<pin name="P4_3/S6"/>
<pin name="P4_2/S7"/>
<pin name="P4_1/S8"/>
<pin name="P4_0/S9"/>
<pin name="P3_7/S10"/>
<pin name="P3_6/S11"/>
<pin name="P3_5/S12"/>
<pin name="P3_4/S13"/>
<pin name="P3_3/S14"/>
<pin name="P3_2/S15"/>
<pin name="P3_1/S16"/>
<pin name="P3_0/S17"/>
<pin name="P2_7/SIFCLKG/S18"/>
<pin name="P2_6/CAOUT/S19"/>
<pin name="P2_5/TA1CLK/S20"/>
<pin name="P2_4/TA1_4/S21"/>
<pin name="P2_3/TA1_3/S22"/>
<pin name="P2_2/TA1_2/S23"/>
<pin name="COM0" direction="out"/>
<pin name="P5_2/COM1"/>
<pin name="P5_3/COM2"/>
<pin name="P5_4/COM3"/>
<pin name="R03" direction="in"/>
<pin name="P5_5/R13"/>
<pin name="P5_6/R23"/>
<pin name="P5_7/R33"/>
<pin name="P2_1/TA1_1"/>
<pin name="P2_0/TA0_2"/>
<pin name="P1_7/CA1"/>
<pin name="P1_6/CA0"/>
<pin name="P1_5/TA0CLK/ACLK"/>
<pin name="P1_4/TA1_0"/>
<pin name="P1_3/TA1_0/SVSOUT"/>
<pin name="P1_2/TA0_1"/>
<pin name="P1_1/TA0_0/MCLK"/>
<pin name="P1_0/TA0_0"/>
<pin name="TDO/TDI"/>
<pin name="TDI/TCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="RST/NMI" direction="in"/>
<pin name="P6_0/SIFCH0"/>
<pin name="P6_1/SIFCH1"/>
<pin name="P6_2/SIFCH2"/>
<pin name="AVSS" direction="pwr"/>
<pin name="DVSS" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="BQ27010">
<pin name="RBI" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="D/C" direction="in"/>
<pin name="HDQ"/>
<pin name="BAT" direction="in"/>
<pin name="SRN" direction="in"/>
<pin name="SRP" direction="in"/>
<pin name="GPIO"/>
<pin name="PGM" direction="in"/>
<pin name="VSSG" direction="pwr"/>
</symbol>
<symbol name="BQ27210">
<pin name="RBI" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="VSS" direction="in"/>
<pin name="SCL" direction="in"/>
<pin name="SDA"/>
<pin name="BAT" direction="in"/>
<pin name="SRN" direction="in"/>
<pin name="SRP" direction="in"/>
<pin name="GPIO"/>
<pin name="PGM" direction="in"/>
<pin name="VSSG" direction="in"/>
</symbol>
<symbol name="PWR-PP10">
<pin name="PP@1" direction="pwr"/>
<pin name="PP@2" direction="pwr"/>
<pin name="PP@3" direction="pwr"/>
<pin name="PP@4" direction="pwr"/>
<pin name="PP@5" direction="pwr"/>
<pin name="PP@6" direction="pwr"/>
<pin name="PP@7" direction="pwr"/>
<pin name="PP@8" direction="pwr"/>
<pin name="PP@9" direction="pwr"/>
<pin name="PP@10" direction="pwr"/>
</symbol>
<symbol name="LM4041">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="LM4041-ADJ">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="FB" direction="pas"/>
</symbol>
<symbol name="MSP430F5437-100">
<pin name="P6_4/A4"/>
<pin name="P6_5/A5"/>
<pin name="P6_6/A6"/>
<pin name="P6_7/A7"/>
<pin name="P7_4/A12"/>
<pin name="P7_5/A13"/>
<pin name="P7_6/A14"/>
<pin name="P7_7/A15"/>
<pin name="P5_0/VREF+/VEREF+"/>
<pin name="P5_1/VREF-/VEREF-"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="P7_0/XIN"/>
<pin name="P7_1/XOUT"/>
<pin name="DVSS1" direction="pwr"/>
<pin name="DVCC1" direction="pwr"/>
<pin name="P1_0/TA0CLK/ACLK"/>
<pin name="P1_1/TA0.0"/>
<pin name="P1_2/TA0.1"/>
<pin name="P1_3/TA0.2"/>
<pin name="P1_4/TA0.3"/>
<pin name="P1_5/TA0.4"/>
<pin name="P1_6/SMCLK"/>
<pin name="P1_7"/>
<pin name="P2_0/TA1CLK/MCLK"/>
<pin name="P2_1/TA1.0"/>
<pin name="P2_2/TA1.1"/>
<pin name="P2_3/TA1.2"/>
<pin name="P2_4/RTCCLK"/>
<pin name="P2_5"/>
<pin name="P2_6/ACLK"/>
<pin name="P2_7/ADC12CLK/DMAE0"/>
<pin name="P3_0/UCB0STE/UCA0CLK"/>
<pin name="P3_1/UCB0SIMO/UCB0SDA"/>
<pin name="P3_2/UCB0SOMI/UCB0SCL"/>
<pin name="P3_3/UCB0CLK/UCA0STE"/>
<pin name="DVSS3" direction="pwr"/>
<pin name="DVCC3" direction="pwr"/>
<pin name="P3_4/UCA0TXD/UCA0SIMO"/>
<pin name="P3_5/UCA0RXD/UCA0SOMI"/>
<pin name="P3_6/UCB1STE/UCA1CLK"/>
<pin name="P3_7/UCB1SIMO/UCB1SDA"/>
<pin name="P4_0/TB0"/>
<pin name="P4_1/TB1"/>
<pin name="P4_2/TB2"/>
<pin name="P4_3/TB3"/>
<pin name="P4_4/TB4"/>
<pin name="P4_5/TB5"/>
<pin name="P4_6/TB6"/>
<pin name="P4_7/TBCLK/SMCLK"/>
<pin name="P5_4/UCB1SOMI/UCB1SCL"/>
<pin name="P5_5/UCB1CLK/UCA1STE"/>
<pin name="P5_6/UCA1TXD/UCA1SIMO"/>
<pin name="P5_7/UCA1RXD/UCA1SOMI"/>
<pin name="P7_2/TBOUTH/SVMOUT"/>
<pin name="P7_3/TA1.2"/>
<pin name="P8_0/TA0.0"/>
<pin name="P8_1/TA0.1"/>
<pin name="P8_2/TA0.2"/>
<pin name="P8_3/TA0.3"/>
<pin name="P8_4/TA0.4"/>
<pin name="VCORE" direction="pwr"/>
<pin name="DVSS2" direction="pwr"/>
<pin name="DVCC2" direction="pwr"/>
<pin name="P8_5/TA1.0"/>
<pin name="P8_6/TA1.1"/>
<pin name="P8_7"/>
<pin name="P9_0/UCB2STE/UCA2CLK"/>
<pin name="P9_1/UCB2SIMO/UCB2SDA"/>
<pin name="P9_2/UCB2SOMI/UCB2SCL"/>
<pin name="P9_3/UCB2CLK/UCA2STE"/>
<pin name="P9_4/UCA2TXD/UCA2SIMO"/>
<pin name="P9_5/UCA2RXD/UCA2SOMI"/>
<pin name="P9_6"/>
<pin name="P9_7"/>
<pin name="P10_0/UCB3STE/UCA3CLK"/>
<pin name="P10_1/UCB3SIMO/UCB3SDA"/>
<pin name="P10_2/UCB3SOMI/UCB3SCL"/>
<pin name="P10_3/UCB3CLK/UCA3STE"/>
<pin name="P10_4/UCA3TXD/UCA3SIMO"/>
<pin name="P10_5/UCA3RXD/UCA3SOMI"/>
<pin name="P10_6"/>
<pin name="P10_7"/>
<pin name="P11_0/ACLK"/>
<pin name="P11_1/MCLK"/>
<pin name="P11_2/SMCLK"/>
<pin name="DVCC4" direction="pwr"/>
<pin name="DVSS4" direction="pwr"/>
<pin name="P5_2/XT2IN"/>
<pin name="P5_3/XT2OUT"/>
<pin name="TEST/SBWTCK" direction="in"/>
<pin name="PJ_0/TDO"/>
<pin name="PJ_1/TDI/TCLK"/>
<pin name="PJ_2/TMS"/>
<pin name="PJ_3/TCK"/>
<pin name="RST/NMI/SBWTDIO"/>
<pin name="P6_0/A0"/>
<pin name="P6_1/A1"/>
<pin name="P6_2/A2"/>
<pin name="P6_3/A3"/>
</symbol>
<symbol name="MSP430F5437-80">
<pin name="P6_4/A4"/>
<pin name="P6_5/A5"/>
<pin name="P6_6/A6"/>
<pin name="P6_7/A7"/>
<pin name="P7_4/A12"/>
<pin name="P7_5/A13"/>
<pin name="P7_6/A14"/>
<pin name="P7_7/A15"/>
<pin name="P5_0/VREF+/VEREF+"/>
<pin name="P5_1/VREF-/VEREF-"/>
<pin name="AVCC" direction="pwr"/>
<pin name="AVSS" direction="pwr"/>
<pin name="P7_0/XIN"/>
<pin name="P7_1/XOUT"/>
<pin name="DVSS1" direction="pwr"/>
<pin name="DVCC1" direction="pwr"/>
<pin name="P1_0/TA0CLK/ACLK"/>
<pin name="P1_1/TA0.0"/>
<pin name="P1_2/TA0.1"/>
<pin name="P1_3/TA0.2"/>
<pin name="P1_4/TA0.3"/>
<pin name="P1_5/TA0.4"/>
<pin name="P1_6/SMCLK"/>
<pin name="P1_7"/>
<pin name="P2_0/TA1CLK/MCLK"/>
<pin name="P2_1/TA1.0"/>
<pin name="P2_2/TA1.1"/>
<pin name="P2_3/TA1.2"/>
<pin name="P2_4/RTCCLK"/>
<pin name="P2_5"/>
<pin name="P2_6/ACLK"/>
<pin name="P2_7/ADC12CLK/DMAE0"/>
<pin name="P3_0/UCB0STE/UCA0CLK"/>
<pin name="P3_1/UCB0SIMO/UCB0SDA"/>
<pin name="P3_2/UCB0SOMI/UCB0SCL"/>
<pin name="P3_3/UCB0CLK/UCA0STE"/>
<pin name="DVSS3" direction="pwr"/>
<pin name="DVCC3" direction="pwr"/>
<pin name="P3_4/UCA0TXD/UCA0SIMO"/>
<pin name="P3_5/UCA0RXD/UCA0SOMI"/>
<pin name="P3_6/UCB1STE/UCA1CLK"/>
<pin name="P3_7/UCB1SIMO/UCB1SDA"/>
<pin name="P4_0/TB0"/>
<pin name="P4_1/TB1"/>
<pin name="P4_2/TB2"/>
<pin name="P4_3/TB3"/>
<pin name="P4_4/TB4"/>
<pin name="P4_5/TB5"/>
<pin name="P4_6/TB6"/>
<pin name="P4_7/TBCLK/SMCLK"/>
<pin name="P5_4/UCB1SOMI/UCB1SCL"/>
<pin name="P5_5/UCB1CLK/UCA1STE"/>
<pin name="P5_6/UCA1TXD/UCA1SIMO"/>
<pin name="P5_7/UCA1RXD/UCA1SOMI"/>
<pin name="P7_2/TBOUTH/SVMOUT"/>
<pin name="P7_3/TA1.2"/>
<pin name="P8_0/TA0.0"/>
<pin name="P8_1/TA0.1"/>
<pin name="P8_2/TA0.2"/>
<pin name="P8_3/TA0.3"/>
<pin name="P8_4/TA0.4"/>
<pin name="VCORE" direction="pwr"/>
<pin name="DVSS2" direction="pwr"/>
<pin name="DVCC2" direction="pwr"/>
<pin name="P8_5/TA1.0"/>
<pin name="P8_6/TA1.1"/>
<pin name="DVCC4" direction="pwr"/>
<pin name="DVSS4" direction="pwr"/>
<pin name="P5_2/XT2IN"/>
<pin name="P5_3/XT2OUT"/>
<pin name="TEST/SBWTCK" direction="in"/>
<pin name="PJ_0/TDO"/>
<pin name="PJ_1/TDI/TCLK"/>
<pin name="PJ_2/TMS"/>
<pin name="PJ_3/TCK"/>
<pin name="!RST!/NMI/SBWTDIO"/>
<pin name="P6_0/A0"/>
<pin name="P6_1/A1"/>
<pin name="P6_2/A2"/>
<pin name="P6_3/A3"/>
</symbol>
<symbol name="MSP430X22X2-DA">
<pin name="TEST/SBWTCK" direction="in"/>
<pin name="DVCC" direction="pwr"/>
<pin name="P2.5/ROSC"/>
<pin name="DVSS" direction="pwr"/>
<pin name="XOUT/P2.7"/>
<pin name="XIN/P2.6"/>
<pin name="!RST!/NMI/SBWTDIO" direction="in"/>
<pin name="P2.0/ACLK/A0"/>
<pin name="P2.1/TAINCLK/SMCLK/A1"/>
<pin name="P2.2/TA0/A2"/>
<pin name="P3.0/UCB0STE/UCA0CLK/A5"/>
<pin name="P3.1/UCB0SIMO/UCB0SDA"/>
<pin name="P3.2/UCB0SOMI/UCB0SCL"/>
<pin name="P3.3/UCB0CLK/UCA0STE"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="P4.0/TB0"/>
<pin name="P4.1/TB1"/>
<pin name="P4.2/TB2"/>
<pin name="P4.3/TB0/A12"/>
<pin name="P4.4/TB1A13"/>
<pin name="P4.5/TB2A14"/>
<pin name="P4.6/TBOUTHA15"/>
<pin name="P4.7/TBCLK"/>
<pin name="P3.4/UCA0TXD/UCA0SIMO"/>
<pin name="P3.5/UCA0RXD/UCA0SOMI"/>
<pin name="P3.6/A6"/>
<pin name="P3.7/A7"/>
<pin name="P2.3/TA1/A3/VREF-/VEREF-"/>
<pin name="P2.4/TA2/A4/VREF+/VEREF+"/>
<pin name="P1.0/TACLK/ADC10CLK"/>
<pin name="P1.1/TA0"/>
<pin name="P1.2/TA1"/>
<pin name="P1.3/TA2"/>
<pin name="P1.4/SMCLK/TCK"/>
<pin name="P1.5/TA0/TMS"/>
<pin name="P1.6/TA1/TDI/TCLK"/>
<pin name="P1.7/TA2/TDO/TDI"/>
</symbol>
<symbol name="MSP430X22X4-DA">
<pin name="TEST/SBWTCK" direction="in"/>
<pin name="DVCC" direction="pwr"/>
<pin name="P2.5/ROSC"/>
<pin name="DVSS" direction="pwr"/>
<pin name="XOUT/P2.7"/>
<pin name="XIN/P2.6"/>
<pin name="!RST!/NMI/SBWTDIO" direction="in"/>
<pin name="P2.0/ACLK/A0/OA0I0"/>
<pin name="P2.1/TAINCLK/SMCLK/A1/OA0O"/>
<pin name="P2.2/TA0/A2/OA0I1"/>
<pin name="P3.0/UCB0STE/UCA0CLK/A5"/>
<pin name="P3.1/UCB0SIMO/UCB0SDA"/>
<pin name="P3.2/UCB0SOMI/UCB0SCL"/>
<pin name="P3.3/UCB0CLK/UCA0STE"/>
<pin name="AVSS" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="P4.0/TB0"/>
<pin name="P4.1/TB1"/>
<pin name="P4.2/TB2"/>
<pin name="P4.3/TB0/A12/OA0O"/>
<pin name="P4.4/TB1A13/OA1O"/>
<pin name="P4.5/TB2A14/OA0I3"/>
<pin name="P4.6/TBOUTHA15/OA1I3"/>
<pin name="P4.7/TBCLK"/>
<pin name="P3.4/UCA0TXD/UCA0SIMO"/>
<pin name="P3.5/UCA0RXD/UCA0SOMI"/>
<pin name="P3.6/A6/OA0I2"/>
<pin name="P3.7/A7/OA1I2"/>
<pin name="P2.3/TA1/A3/VREF-/VEREF-/OA1I1/OA1O"/>
<pin name="P2.4/TA2/A4/VREF+/VEREF+/OA1I0"/>
<pin name="P1.0/TACLK/ADC10CLK"/>
<pin name="P1.1/TA0"/>
<pin name="P1.2/TA1"/>
<pin name="P1.3/TA2"/>
<pin name="P1.4/SMCLK/TCK"/>
<pin name="P1.5/TA0/TMS"/>
<pin name="P1.6/TA1/TDI/TCLK"/>
<pin name="P1.7/TA2/TDO/TDI"/>
</symbol>
<symbol name="TPS773XX">
<pin name="FB/SENSE" direction="in"/>
<pin name="!RESET" direction="out"/>
<pin name="!EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="IN@1" direction="in"/>
<pin name="IN@2" direction="in"/>
<pin name="OUT@1" direction="out"/>
<pin name="OUT@2" direction="pas"/>
</symbol>
<symbol name="TPS774XX">
<pin name="FB/SENSE" direction="in"/>
<pin name="PG" direction="out"/>
<pin name="!EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="IN@1" direction="in"/>
<pin name="IN@2" direction="in"/>
<pin name="OUT@1" direction="out"/>
<pin name="OUT@2" direction="pas"/>
</symbol>
<symbol name="TPS6300X">
<pin name="L1" direction="pas"/>
<pin name="L2" direction="pas"/>
<pin name="VIN" direction="in"/>
<pin name="VINA" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="PS/SYNC" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="PGND" direction="pwr"/>
</symbol>
<symbol name="THERMAL3">
<pin name="TH@1" direction="pas"/>
<pin name="TH@2" direction="pas"/>
<pin name="TH@3" direction="pas"/>
</symbol>
<symbol name="UC3637N">
<pin name="+VS" direction="in"/>
<pin name="+AIN" direction="in"/>
<pin name="-AIN" direction="in"/>
<pin name="ISET" direction="in"/>
<pin name="+VTH" direction="in"/>
<pin name="CT" direction="pas"/>
<pin name="-VTH" direction="in"/>
<pin name="-E/A" direction="in"/>
<pin name="+E/A" direction="in"/>
<pin name="-VS" direction="in"/>
<pin name="E/A_OUT" direction="out"/>
<pin name="AOUT" direction="out"/>
<pin name="BOUT" direction="out"/>
<pin name="+BIN" direction="in"/>
<pin name="-BIN" direction="in"/>
<pin name="SH_DOWN" direction="in"/>
<pin name="-C/L" direction="in"/>
<pin name="+C/L" direction="in"/>
</symbol>
<symbol name="TPA6132A2">
<pin name="INR+" direction="in"/>
<pin name="INR-" direction="in"/>
<pin name="INL+" direction="in"/>
<pin name="INL-" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GO" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="VDD" direction="pwr"/>
<pin name="HPVDD" direction="pas"/>
<pin name="OUTR" direction="out"/>
<pin name="OUTL" direction="out"/>
<pin name="SGND" direction="pwr"/>
<pin name="HPVSS" direction="pas"/>
<pin name="CPN" direction="pas"/>
<pin name="CPP" direction="pas"/>
<pin name="PGND" direction="pwr"/>
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="TPA3123D2">
<pin name="LIN" direction="in"/>
<pin name="RIN" direction="in"/>
<pin name="BYPASS" direction="in"/>
<pin name="AGND@1" direction="in"/>
<pin name="AVCC@1" direction="in"/>
<pin name="!SD" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="PVCCL@1" direction="in"/>
<pin name="PVCCR@1" direction="in"/>
<pin name="GAIN0" direction="in"/>
<pin name="GAIN1" direction="in"/>
<pin name="VCLAMP" direction="in"/>
<pin name="BSR" direction="pas"/>
<pin name="BSL" direction="pas"/>
<pin name="ROUT" direction="out"/>
<pin name="LOUT" direction="out"/>
<pin name="PGNDR@1" direction="in"/>
<pin name="PGNDL@1" direction="in"/>
<pin name="PGNDR@2" direction="in"/>
<pin name="PGNDL@2" direction="in"/>
<pin name="PVCCR@2" direction="in"/>
<pin name="PVCCL@2" direction="in"/>
<pin name="AGND@2" direction="in"/>
<pin name="AVCC@2" direction="in"/>
</symbol>
<symbol name="EXP19">
<pin name="EXP" direction="pas"/>
<pin name="EXP@1" direction="pas"/>
<pin name="EXP@2" direction="pas"/>
<pin name="EXP@3" direction="pas"/>
<pin name="EXP@4" direction="pas"/>
<pin name="EXP@5" direction="pas"/>
<pin name="EXP@6" direction="pas"/>
<pin name="EXP@7" direction="pas"/>
<pin name="EXP@8" direction="pas"/>
<pin name="EXP@9" direction="pas"/>
<pin name="EXP@10" direction="pas"/>
<pin name="EXP@11" direction="pas"/>
<pin name="EXP@12" direction="pas"/>
<pin name="EXP@13" direction="pas"/>
<pin name="EXP@14" direction="pas"/>
<pin name="EXP@15" direction="pas"/>
<pin name="EXP@16" direction="pas"/>
<pin name="EXP@17" direction="pas"/>
<pin name="EXP@18" direction="pas"/>
</symbol>
<symbol name="MSP430FG437">
<pin name="DVCC1" direction="pwr"/>
<pin name="P6_3/A3/OA1I1/OA1O"/>
<pin name="P6_4/A4/OA1I0"/>
<pin name="P6_5/A5/OA2I1/OA2O"/>
<pin name="P6_6/A6/DAC0/OA2I0"/>
<pin name="P6_7/A7/DAC1/SVSIN"/>
<pin name="VREF+" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="VEREF+/DAC0"/>
<pin name="VREF-/VEREF-" direction="in"/>
<pin name="P5_1/S0/A12/DAC1"/>
<pin name="P5_0/S1/A13"/>
<pin name="P4_7/S2/A14"/>
<pin name="P4_6/S3/A15"/>
<pin name="P4_5/S4"/>
<pin name="P4_4/S5"/>
<pin name="P4_3/S6"/>
<pin name="P4_2/S7"/>
<pin name="P4_1/S8"/>
<pin name="P4_0/S9"/>
<pin name="S10" direction="out"/>
<pin name="S11" direction="out"/>
<pin name="S12" direction="out"/>
<pin name="S13" direction="out"/>
<pin name="S14" direction="out"/>
<pin name="S15" direction="out"/>
<pin name="S16" direction="out"/>
<pin name="S17" direction="out"/>
<pin name="P2_7/ADC12CLK/S18"/>
<pin name="P2_6/CAOUT/S19"/>
<pin name="S20" direction="out"/>
<pin name="S21" direction="out"/>
<pin name="S22" direction="out"/>
<pin name="S23" direction="out"/>
<pin name="P3_7/S24"/>
<pin name="P3_6/S25/DMAE0"/>
<pin name="P3_5/S26"/>
<pin name="P3_4/S27"/>
<pin name="P3_3/UCLK0/S28"/>
<pin name="P3_2/SOMI0/S29"/>
<pin name="P3_1/SIMO0/S30"/>
<pin name="P3_0/STE0/S31"/>
<pin name="COM0" direction="out"/>
<pin name="P5_2/COM1"/>
<pin name="P5_3/COM2"/>
<pin name="P5_4/COM3"/>
<pin name="R03" direction="in"/>
<pin name="P5_5/R13"/>
<pin name="P5_6/R23"/>
<pin name="P5_7/R33"/>
<pin name="DVCC2" direction="pwr"/>
<pin name="DVSS2" direction="pwr"/>
<pin name="P2_5/URXD0"/>
<pin name="P2_4/UTXD0"/>
<pin name="P2_3/TB2"/>
<pin name="P2_2/TB1"/>
<pin name="P2_1/TB0"/>
<pin name="P2_0/TA2"/>
<pin name="P1_7/CA13"/>
<pin name="P1_6/CA0"/>
<pin name="P1_5/TACLK/ACLK"/>
<pin name="P1_4/TBCLK/SMCLK"/>
<pin name="P1_3/TBOUTH/SVSOUT"/>
<pin name="P1_2/TA1"/>
<pin name="P1_1/TA0/MCLK"/>
<pin name="P1_0/TA0"/>
<pin name="XT2OUT" direction="out"/>
<pin name="XT2IN" direction="in"/>
<pin name="TDO/TDI"/>
<pin name="TDI/TCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="RST/NMI" direction="in"/>
<pin name="P6_0/A0/OA0I0"/>
<pin name="P6_1/A1/OA0O"/>
<pin name="P6_2/A2/OA0I1"/>
<pin name="AVSS" direction="pwr"/>
<pin name="DVSS1" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
</symbol>
<symbol name="TPS6108">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="FSW" direction="in"/>
<pin name="SS" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="L" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="FB" direction="in"/>
<pin name="PGND" direction="in"/>
<pin name="SW" direction="pas"/>
</symbol>
<symbol name="EXP-3">
<pin name="EXP@1" direction="in"/>
<pin name="EXP@2" direction="in"/>
<pin name="EXP@3" direction="in"/>
</symbol>
<symbol name="SRC4392">
<pin name="SDINA" direction="in"/>
<pin name="SDINB" direction="in"/>
<pin name="SDOUTA" direction="out"/>
<pin name="SDOUTB" direction="out"/>
<pin name="LRCKA"/>
<pin name="LRCKB"/>
<pin name="BCKA"/>
<pin name="BCKB"/>
<pin name="RXCKO" direction="out"/>
<pin name="!LOCK" direction="out"/>
<pin name="RX1+" direction="in"/>
<pin name="RX1-" direction="in"/>
<pin name="RX2+" direction="in"/>
<pin name="RX2-" direction="in"/>
<pin name="RX3+" direction="in"/>
<pin name="RX3-" direction="in"/>
<pin name="RX4+" direction="in"/>
<pin name="RX4-" direction="in"/>
<pin name="TX+" direction="out"/>
<pin name="TX-" direction="out"/>
<pin name="AESOUT" direction="out"/>
<pin name="BLS"/>
<pin name="SYNC" direction="out"/>
<pin name="!RDY" direction="out"/>
<pin name="MUTE" direction="in"/>
<pin name="CPM" direction="in"/>
<pin name="!CS!/A0" direction="in"/>
<pin name="CCLK/SCL" direction="in"/>
<pin name="CDIN/A1" direction="in"/>
<pin name="CDOUT/SDA"/>
<pin name="!INT" direction="out"/>
<pin name="!RST" direction="in"/>
<pin name="GPO1" direction="out"/>
<pin name="GPO2" direction="out"/>
<pin name="GPO3" direction="out"/>
<pin name="GPO4" direction="out"/>
<pin name="MCLK" direction="in"/>
<pin name="RXCKI" direction="in"/>
<pin name="VDD18" direction="in"/>
<pin name="DGND1" direction="in"/>
<pin name="VDD33" direction="in"/>
<pin name="DGND2" direction="in"/>
<pin name="VIO" direction="in"/>
<pin name="DGND3" direction="in"/>
<pin name="VCC" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="BGND" direction="in"/>
</symbol>
<symbol name="SRC4382">
<pin name="RX1+" direction="in"/>
<pin name="RX1-" direction="in"/>
<pin name="RX2+" direction="in"/>
<pin name="RX2-" direction="in"/>
<pin name="RX3+" direction="in"/>
<pin name="RX3-" direction="in"/>
<pin name="RX4+" direction="in"/>
<pin name="RX4-" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="!LOCK" direction="out"/>
<pin name="RXCKO" direction="out"/>
<pin name="RXCKI" direction="in"/>
<pin name="MUTE" direction="in"/>
<pin name="!RDY" direction="out"/>
<pin name="DGND1" direction="pwr"/>
<pin name="VDD18" direction="pwr"/>
<pin name="CPM" direction="in"/>
<pin name="!CS!/A0" direction="in"/>
<pin name="CCLK/SCL" direction="in"/>
<pin name="CDIN/A1" direction="in"/>
<pin name="CDOUT/SDA"/>
<pin name="!INT" direction="out"/>
<pin name="!RST" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="GPO1" direction="out"/>
<pin name="GPO2" direction="out"/>
<pin name="GPO3" direction="out"/>
<pin name="GPO4" direction="out"/>
<pin name="DGND2" direction="pwr"/>
<pin name="TX-" direction="out"/>
<pin name="TX+" direction="out"/>
<pin name="VDD33" direction="pwr"/>
<pin name="AESOUT" direction="out"/>
<pin name="BLS"/>
<pin name="SYNC" direction="out"/>
<pin name="BCKA"/>
<pin name="LRCKA"/>
<pin name="SDINA" direction="in"/>
<pin name="SDOUTA" direction="out"/>
<pin name="NC" direction="nc"/>
<pin name="VIO" direction="pwr"/>
<pin name="DGND3" direction="pwr"/>
<pin name="BGND" direction="pwr"/>
<pin name="SDOUTB" direction="out"/>
<pin name="SDINB" direction="in"/>
<pin name="LRCKB"/>
<pin name="BCKB"/>
</symbol>
<symbol name="DIT4192-HARDWARE-MODE">
<pin name="CSS" direction="in"/>
<pin name="COPY/C" direction="in"/>
<pin name="L" direction="in"/>
<pin name="CLK1" direction="in"/>
<pin name="CLK0" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="VIO" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="FMT0" direction="in"/>
<pin name="FMT1" direction="in"/>
<pin name="SCLK"/>
<pin name="SYNC"/>
<pin name="SDATA" direction="in"/>
<pin name="M/!S" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="TX-" direction="out"/>
<pin name="TX+" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="MDAT" direction="in"/>
<pin name="MONO" direction="in"/>
<pin name="!AUDIO" direction="in"/>
<pin name="!EMPH" direction="in"/>
<pin name="BLSM" direction="in"/>
<pin name="BLS"/>
<pin name="V" direction="in"/>
<pin name="U" direction="in"/>
<pin name="MODE" direction="in"/>
</symbol>
<symbol name="DIT4192-SOFTWARE-MODE">
<pin name="NC" direction="nc"/>
<pin name="CDOUT" direction="out"/>
<pin name="CCLK" direction="in"/>
<pin name="CDIN" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="VIO" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="RXP" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="SCLK"/>
<pin name="SYNC"/>
<pin name="SDATA" direction="in"/>
<pin name="NC@2" direction="nc"/>
<pin name="!RST" direction="in"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="TX-" direction="out"/>
<pin name="TX+" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="!INT" direction="oc"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="BLS"/>
<pin name="NC@7" direction="nc"/>
<pin name="U" direction="in"/>
<pin name="MODE" direction="in"/>
</symbol>
<symbol name="TMS320C6720-1">
<pin name="AHCLKR0/AHCLKR1"/>
<pin name="ACLKR0"/>
<pin name="AFSR0"/>
<pin name="AHCLKX0/AHCLKX2"/>
<pin name="ACLKX0"/>
<pin name="AFSX0"/>
<pin name="ACLKR1"/>
<pin name="AFSR1"/>
<pin name="AHCLKX1"/>
<pin name="ACLKX1"/>
<pin name="AFSX1"/>
<pin name="AMUTE1" direction="out"/>
<pin name="AHCLKR2"/>
<pin name="ACLKR2"/>
<pin name="AFSR2"/>
<pin name="ACLKX2"/>
<pin name="AFSX2"/>
<pin name="AMUTE2/HINT" direction="out"/>
<pin name="SPI0_SOMI/I2C0_SDA"/>
<pin name="SPI0_SIMO"/>
<pin name="SPI0_CLK/I2C0_SCL"/>
<pin name="SPI0_SCS/I2C1_SCL"/>
<pin name="SPI0_ENA/I2C1_SDA"/>
<pin name="OSCIN" direction="in"/>
<pin name="OSCOUT" direction="out"/>
<pin name="OSCVDD" direction="pwr"/>
<pin name="OSCVSS" direction="pwr"/>
<pin name="CLKIN" direction="in"/>
<pin name="PLLHV" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="hiz"/>
<pin name="TRST" direction="in"/>
<pin name="EMU0"/>
<pin name="EMU1"/>
<pin name="AMUTE0" direction="out"/>
</symbol>
<symbol name="TMS320C6720-AXI">
<pin name="AXR00"/>
<pin name="AXR01"/>
<pin name="AXR02"/>
<pin name="AXR03"/>
<pin name="AXR04"/>
<pin name="AXR05/SPI1_SCS"/>
<pin name="AXR06/SPI1_ENA"/>
<pin name="AXR07/SPI1_CLK"/>
<pin name="AXR08/AXR15/SPI1_SOMI"/>
<pin name="AXR09/AXR14/SPI1_SIMO"/>
<pin name="AXR010/AXR13"/>
<pin name="AXR011/AXR12"/>
<pin name="AXR012/AXR11"/>
<pin name="AXR013/AXR10"/>
<pin name="AXR014/AXR21"/>
<pin name="AXR015/AXR20"/>
</symbol>
<symbol name="TMS320C6720-EM">
<pin name="EM_A0" direction="out"/>
<pin name="EM_A1" direction="out"/>
<pin name="EM_A2" direction="out"/>
<pin name="EM_A3" direction="out"/>
<pin name="EM_A4" direction="out"/>
<pin name="EM_A5" direction="out"/>
<pin name="EM_A6" direction="out"/>
<pin name="EM_A7" direction="out"/>
<pin name="EM_A8" direction="out"/>
<pin name="EM_A9" direction="out"/>
<pin name="EM_A10" direction="out"/>
<pin name="EM_A11" direction="out"/>
<pin name="EM_A12" direction="out"/>
<pin name="EM_BA0" direction="out"/>
<pin name="EM_BA1" direction="out"/>
<pin name="EM_CS0" direction="out"/>
<pin name="EM_CS2" direction="out"/>
<pin name="EM_CAS" direction="out"/>
<pin name="EM_RAS" direction="out"/>
<pin name="EM_WE" direction="out"/>
<pin name="EM_CKE" direction="out"/>
<pin name="EM_CLK" direction="out"/>
<pin name="EM_WE_DQM0" direction="out"/>
<pin name="EM_WE_DQM1" direction="out"/>
<pin name="EM_WE_DQM2" direction="out"/>
<pin name="EM_WE_DQM3" direction="out"/>
<pin name="EM_OE" direction="out"/>
<pin name="EM_RW" direction="out"/>
<pin name="EM_WAIT" direction="in"/>
<pin name="EM_D0"/>
<pin name="EM_D1"/>
<pin name="EM_D2"/>
<pin name="EM_D3"/>
<pin name="EM_D4"/>
<pin name="EM_D5"/>
<pin name="EM_D6"/>
<pin name="EM_D7"/>
<pin name="EM_D8"/>
<pin name="EM_D9"/>
<pin name="EM_D10"/>
<pin name="EM_D11"/>
<pin name="EM_D12"/>
<pin name="EM_D13"/>
<pin name="EM_D14"/>
<pin name="EM_D15"/>
<pin name="EM_D16/UHPI_HA0"/>
<pin name="EM_D17/UHPI_HA1"/>
<pin name="EM_D18/UHPI_HA2"/>
<pin name="EM_D19/UHPI_HA3"/>
<pin name="EM_D20/UHPI_HA4"/>
<pin name="EM_D21/UHPI_HA5"/>
<pin name="EM_D22/UHPI_HA6"/>
<pin name="EM_D23/UHPI_HA7"/>
<pin name="EM_D24/UHPI_HA8"/>
<pin name="EM_D25/UHPI_HA9"/>
<pin name="EM_D26/UHPI_HA10"/>
<pin name="EM_D27/UHPI_HA11"/>
<pin name="EM_D28/UHPI_HA12"/>
<pin name="EM_D29/UHPI_HA13"/>
<pin name="EM_D30/UHPI_HA14"/>
<pin name="EM_D31/UHPI_HA15"/>
</symbol>
<symbol name="TMS320C6720-UHPI">
<pin name="UHPI_HD0"/>
<pin name="UHPI_HD1"/>
<pin name="UHPI_HD2"/>
<pin name="UHPI_HD3"/>
<pin name="UHPI_HD4"/>
<pin name="UHPI_HD5"/>
<pin name="UHPI_HD6"/>
<pin name="UHPI_HD7"/>
<pin name="UHPI_HD8"/>
<pin name="UHPI_HD9"/>
<pin name="UHPI_HD10"/>
<pin name="UHPI_HD11"/>
<pin name="UHPI_HD12"/>
<pin name="UHPI_HD13"/>
<pin name="UHPI_HD14"/>
<pin name="UHPI_HD15"/>
<pin name="UHPI_HD16/HHWIL"/>
<pin name="UHPI_HD17"/>
<pin name="UHPI_HD18"/>
<pin name="UHPI_HD19"/>
<pin name="UHPI_HD20"/>
<pin name="UHPI_HD21"/>
<pin name="UHPI_HD22"/>
<pin name="UHPI_HD23"/>
<pin name="UHPI_HD24"/>
<pin name="UHPI_HD25"/>
<pin name="UHPI_HD26"/>
<pin name="UHPI_HD27"/>
<pin name="UHPI_HD28"/>
<pin name="UHPI_HD29"/>
<pin name="UHPI_HD30"/>
<pin name="UHPI_HD31"/>
<pin name="UHPI_HBE0" direction="in"/>
<pin name="UHPI_HBE1" direction="in"/>
<pin name="UHPI_HBE2" direction="in"/>
<pin name="UHPI_HBE3" direction="in"/>
<pin name="UHPI_HCNTL0" direction="in"/>
<pin name="UHPI_HCNTL1" direction="in"/>
<pin name="UHPI_HAS" direction="in"/>
<pin name="UHPI_HRW" direction="in"/>
<pin name="UHPI_HDS1" direction="in"/>
<pin name="UHPI_HDS2" direction="in"/>
<pin name="UHPI_HCS" direction="in"/>
<pin name="UHPI_HRDY" direction="out"/>
</symbol>
<symbol name="TMS320C6720-CVDD">
<pin name="CVDD" direction="pwr"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="CVDD@7" direction="pwr"/>
<pin name="CVDD@8" direction="pwr"/>
<pin name="CVDD@9" direction="pwr"/>
<pin name="CVDD@10" direction="pwr"/>
<pin name="CVDD@11" direction="pwr"/>
<pin name="CVDD@12" direction="pwr"/>
<pin name="CVDD@13" direction="pwr"/>
<pin name="CVDD@14" direction="pwr"/>
<pin name="CVDD@15" direction="pwr"/>
<pin name="CVDD@16" direction="pwr"/>
<pin name="CVDD@17" direction="pwr"/>
<pin name="CVDD@18" direction="pwr"/>
<pin name="CVDD@19" direction="pwr"/>
</symbol>
<symbol name="TMS320C6720-DVDD">
<pin name="DVDD" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="DVDD@7" direction="pwr"/>
<pin name="DVDD@8" direction="pwr"/>
<pin name="DVDD@9" direction="pwr"/>
<pin name="DVDD@10" direction="pwr"/>
<pin name="DVDD@11" direction="pwr"/>
<pin name="DVDD@12" direction="pwr"/>
<pin name="DVDD@13" direction="pwr"/>
<pin name="DVDD@14" direction="pwr"/>
<pin name="DVDD@15" direction="pwr"/>
<pin name="DVDD@16" direction="pwr"/>
<pin name="DVDD@17" direction="pwr"/>
<pin name="DVDD@18" direction="pwr"/>
<pin name="DVDD@19" direction="pwr"/>
</symbol>
<symbol name="TMS320C6720-VSS">
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
<pin name="VSS@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="VSS@45" direction="pwr"/>
<pin name="VSS@46" direction="pwr"/>
<pin name="VSS@47" direction="pwr"/>
<pin name="VSS@48" direction="pwr"/>
<pin name="VSS@49" direction="pwr"/>
<pin name="VSS@50" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VSS@52" direction="pwr"/>
<pin name="VSS@53" direction="pwr"/>
<pin name="VSS@54" direction="pwr"/>
<pin name="VSS@55" direction="pwr"/>
<pin name="VSS@56" direction="pwr"/>
</symbol>
<symbol name="TMS320C6720-QFP-A">
<pin name="AHCLKR0/AHCLKR1"/>
<pin name="ACLKR0"/>
<pin name="AFSR0"/>
<pin name="AHCLKX0/AHCLKX2"/>
<pin name="ACLKX0"/>
<pin name="AFSX0"/>
<pin name="AMUTE0" direction="out"/>
<pin name="AXR00"/>
<pin name="AXR01"/>
<pin name="AXR02"/>
<pin name="AXR03"/>
<pin name="AXR04"/>
<pin name="AXR05/SPI1_SCS"/>
<pin name="AXR06/SPI1_ENA"/>
<pin name="AXR07/SPI1_CLK"/>
<pin name="AXR08/AXR15/SPI1_SOMI"/>
<pin name="AXR09/AXR14/SPI1_SIMO"/>
<pin name="AXR010/AXR13"/>
<pin name="AXR011/AXR12"/>
<pin name="AXR012/AXR11"/>
<pin name="AXR013/AXR10"/>
<pin name="AXR014/AXR21"/>
<pin name="AXR015/AXR20"/>
<pin name="ACLKR1"/>
<pin name="AFSR1"/>
<pin name="AHCLKX1"/>
<pin name="ACLKX1"/>
<pin name="AFSX1"/>
<pin name="AMUTE1" direction="out"/>
<pin name="SPI0_SOMI/I2C0_SDA"/>
<pin name="SPI0_SIMO"/>
<pin name="SPI0_CLK/I2C0_SCL"/>
<pin name="SPI0_SCS/I2C1_SCL"/>
<pin name="SPI0_ENA/I2C1_SDA"/>
<pin name="OSCIN" direction="in"/>
<pin name="OSCOUT" direction="out"/>
<pin name="OSCVDD" direction="pwr"/>
<pin name="OSCVSS" direction="pwr"/>
<pin name="CLKIN" direction="in"/>
<pin name="PLLHV" direction="pwr"/>
<pin name="RESET" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="hiz"/>
<pin name="TRST" direction="in"/>
<pin name="EMU0"/>
<pin name="EMU1"/>
</symbol>
<symbol name="TMS320C6720-QFP-EM">
<pin name="EM_A0" direction="out"/>
<pin name="EM_A1" direction="out"/>
<pin name="EM_A2" direction="out"/>
<pin name="EM_A3" direction="out"/>
<pin name="EM_A4" direction="out"/>
<pin name="EM_A5" direction="out"/>
<pin name="EM_A6" direction="out"/>
<pin name="EM_A7" direction="out"/>
<pin name="EM_A8" direction="out"/>
<pin name="EM_A9" direction="out"/>
<pin name="EM_A10" direction="out"/>
<pin name="EM_A11" direction="out"/>
<pin name="EM_BA0" direction="out"/>
<pin name="EM_BA1" direction="out"/>
<pin name="EM_CS0" direction="out"/>
<pin name="EM_CS2" direction="out"/>
<pin name="EM_CAS" direction="out"/>
<pin name="EM_RAS" direction="out"/>
<pin name="EM_WE" direction="out"/>
<pin name="EM_CKE" direction="out"/>
<pin name="EM_CLK" direction="out"/>
<pin name="EM_WE_DQM0" direction="out"/>
<pin name="EM_WE_DQM1" direction="out"/>
<pin name="EM_OE" direction="out"/>
<pin name="EM_RW" direction="out"/>
<pin name="EM_D0"/>
<pin name="EM_D1"/>
<pin name="EM_D2"/>
<pin name="EM_D3"/>
<pin name="EM_D4"/>
<pin name="EM_D5"/>
<pin name="EM_D6"/>
<pin name="EM_D7"/>
<pin name="EM_D8"/>
<pin name="EM_D9"/>
<pin name="EM_D10"/>
<pin name="EM_D11"/>
<pin name="EM_D12"/>
<pin name="EM_D13"/>
<pin name="EM_D14"/>
<pin name="EM_D15"/>
</symbol>
<symbol name="TMS320C6720-QFP-CVDD">
<pin name="CVDD" direction="pwr"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="CVDD@7" direction="pwr"/>
<pin name="CVDD@8" direction="pwr"/>
<pin name="CVDD@9" direction="pwr"/>
<pin name="CVDD@10" direction="pwr"/>
<pin name="CVDD@11" direction="pwr"/>
<pin name="CVDD@12" direction="pwr"/>
<pin name="CVDD@13" direction="pwr"/>
<pin name="CVDD@14" direction="pwr"/>
</symbol>
<symbol name="TMS320C6720-QFP-DVDD">
<pin name="DVDD" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="DVDD@7" direction="pwr"/>
<pin name="DVDD@8" direction="pwr"/>
<pin name="DVDD@9" direction="pwr"/>
<pin name="DVDD@10" direction="pwr"/>
<pin name="DVDD@11" direction="pwr"/>
<pin name="DVDD@12" direction="pwr"/>
</symbol>
<symbol name="TMS320C6720-QFP-VSS">
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
</symbol>
<symbol name="EXP-100">
<pin name="EXP@1" direction="in"/>
<pin name="EXP@2" direction="in"/>
<pin name="EXP@3" direction="in"/>
<pin name="EXP@4" direction="in"/>
<pin name="EXP@5" direction="in"/>
<pin name="EXP@6" direction="in"/>
<pin name="EXP@7" direction="in"/>
<pin name="EXP@8" direction="in"/>
<pin name="EXP@9" direction="in"/>
<pin name="EXP@10" direction="in"/>
<pin name="EXP@11" direction="in"/>
<pin name="EXP@12" direction="in"/>
<pin name="EXP@13" direction="in"/>
<pin name="EXP@14" direction="in"/>
<pin name="EXP@15" direction="in"/>
<pin name="EXP@16" direction="in"/>
<pin name="EXP@17" direction="in"/>
<pin name="EXP@18" direction="in"/>
<pin name="EXP@19" direction="in"/>
<pin name="EXP@20" direction="in"/>
<pin name="EXP@21" direction="in"/>
<pin name="EXP@22" direction="in"/>
<pin name="EXP@23" direction="in"/>
<pin name="EXP@24" direction="in"/>
<pin name="EXP@25" direction="in"/>
<pin name="EXP@26" direction="in"/>
<pin name="EXP@27" direction="in"/>
<pin name="EXP@28" direction="in"/>
<pin name="EXP@29" direction="in"/>
<pin name="EXP@30" direction="in"/>
<pin name="EXP@31" direction="in"/>
<pin name="EXP@32" direction="in"/>
<pin name="EXP@33" direction="in"/>
<pin name="EXP@34" direction="in"/>
<pin name="EXP@35" direction="in"/>
<pin name="EXP@36" direction="in"/>
<pin name="EXP@37" direction="in"/>
<pin name="EXP@38" direction="in"/>
<pin name="EXP@39" direction="in"/>
<pin name="EXP@40" direction="in"/>
<pin name="EXP@41" direction="in"/>
<pin name="EXP@42" direction="in"/>
<pin name="EXP@43" direction="in"/>
<pin name="EXP@44" direction="in"/>
<pin name="EXP@45" direction="in"/>
<pin name="EXP@46" direction="in"/>
<pin name="EXP@47" direction="in"/>
<pin name="EXP@48" direction="in"/>
<pin name="EXP@49" direction="in"/>
<pin name="EXP@50" direction="in"/>
<pin name="EXP@51" direction="in"/>
<pin name="EXP@52" direction="in"/>
<pin name="EXP@53" direction="in"/>
<pin name="EXP@54" direction="in"/>
<pin name="EXP@55" direction="in"/>
<pin name="EXP@56" direction="in"/>
<pin name="EXP@57" direction="in"/>
<pin name="EXP@58" direction="in"/>
<pin name="EXP@59" direction="in"/>
<pin name="EXP@60" direction="in"/>
<pin name="EXP@61" direction="in"/>
<pin name="EXP@62" direction="in"/>
<pin name="EXP@63" direction="in"/>
<pin name="EXP@64" direction="in"/>
<pin name="EXP@65" direction="in"/>
<pin name="EXP@66" direction="in"/>
<pin name="EXP@67" direction="in"/>
<pin name="EXP@68" direction="in"/>
<pin name="EXP@69" direction="in"/>
<pin name="EXP@70" direction="in"/>
<pin name="EXP@71" direction="in"/>
<pin name="EXP@72" direction="in"/>
<pin name="EXP@73" direction="in"/>
<pin name="EXP@74" direction="in"/>
<pin name="EXP@75" direction="in"/>
<pin name="EXP@76" direction="in"/>
<pin name="EXP@77" direction="in"/>
<pin name="EXP@78" direction="in"/>
<pin name="EXP@79" direction="in"/>
<pin name="EXP@80" direction="in"/>
<pin name="EXP@81" direction="in"/>
<pin name="EXP@82" direction="in"/>
<pin name="EXP@83" direction="in"/>
<pin name="EXP@84" direction="in"/>
<pin name="EXP@85" direction="in"/>
<pin name="EXP@86" direction="in"/>
<pin name="EXP@87" direction="in"/>
<pin name="EXP@88" direction="in"/>
<pin name="EXP@89" direction="in"/>
<pin name="EXP@90" direction="in"/>
<pin name="EXP@91" direction="in"/>
<pin name="EXP@92" direction="in"/>
<pin name="EXP@93" direction="in"/>
<pin name="EXP@94" direction="in"/>
<pin name="EXP@95" direction="in"/>
<pin name="EXP@96" direction="in"/>
<pin name="EXP@97" direction="in"/>
<pin name="EXP@98" direction="in"/>
<pin name="EXP@99" direction="in"/>
<pin name="EXP@100" direction="in"/>
</symbol>
<symbol name="EXP1">
<pin name="EXP" direction="in"/>
</symbol>
<symbol name="DIX4192">
<pin name="RX1+" direction="in"/>
<pin name="RX1-" direction="in"/>
<pin name="RX2+" direction="in"/>
<pin name="RX2-" direction="in"/>
<pin name="RX3+" direction="in"/>
<pin name="RX3-" direction="in"/>
<pin name="RX4+" direction="in"/>
<pin name="RX4-" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="LOCK" direction="out"/>
<pin name="RXCKO" direction="out"/>
<pin name="RXCKI" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="DGND1" direction="pwr"/>
<pin name="VDD18" direction="pwr"/>
<pin name="CPM" direction="in"/>
<pin name="CS/A0" direction="in"/>
<pin name="CCLK/SCL" direction="in"/>
<pin name="CDIN/A1" direction="in"/>
<pin name="CDOUT/SDA"/>
<pin name="INT" direction="out"/>
<pin name="RST" direction="in"/>
<pin name="MCLK" direction="in"/>
<pin name="GPO1" direction="out"/>
<pin name="GPO2" direction="out"/>
<pin name="GPO3" direction="out"/>
<pin name="GPO4" direction="out"/>
<pin name="DGND2" direction="pwr"/>
<pin name="TX" direction="out"/>
<pin name="TX+" direction="out"/>
<pin name="VDD33" direction="pwr"/>
<pin name="AESOUT" direction="out"/>
<pin name="BLS"/>
<pin name="SYNC" direction="out"/>
<pin name="BCKA"/>
<pin name="LRCKA"/>
<pin name="SDINA" direction="in"/>
<pin name="SDOUTA" direction="out"/>
<pin name="NC@2" direction="nc"/>
<pin name="VIO" direction="pwr"/>
<pin name="DGND3" direction="pwr"/>
<pin name="BGND" direction="pwr"/>
<pin name="SDOUTB" direction="out"/>
<pin name="SDINB" direction="in"/>
<pin name="LRCKB"/>
<pin name="BCKB"/>
</symbol>
<symbol name="ADS1278">
<pin name="AINP2" direction="in"/>
<pin name="AINN2" direction="in"/>
<pin name="AINP1" direction="in"/>
<pin name="AINN1" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="TEST0" direction="in"/>
<pin name="TEST1" direction="in"/>
<pin name="CLKDIV" direction="in"/>
<pin name="!SYNC" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT8" direction="out"/>
<pin name="DOUT7" direction="out"/>
<pin name="DOUT6" direction="out"/>
<pin name="DOUT5" direction="out"/>
<pin name="DOUT4" direction="out"/>
<pin name="DOUT3" direction="out"/>
<pin name="DOUT2" direction="out"/>
<pin name="DOUT1" direction="out"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="SCLK"/>
<pin name="!DRDY!/FSYNC"/>
<pin name="FORMAT2" direction="in"/>
<pin name="FORMAT1" direction="in"/>
<pin name="FORMAT0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="!PWDN8" direction="in"/>
<pin name="!PWDN7" direction="in"/>
<pin name="!PWDN6" direction="in"/>
<pin name="!PWDN5" direction="in"/>
<pin name="!PWDN4" direction="in"/>
<pin name="!PWDN3" direction="in"/>
<pin name="!PWDN2" direction="in"/>
<pin name="!PWDN1" direction="in"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="AINP8" direction="in"/>
<pin name="AINN8" direction="in"/>
<pin name="AINP7" direction="in"/>
<pin name="AINN7" direction="in"/>
<pin name="AINP6" direction="in"/>
<pin name="AINN6" direction="in"/>
<pin name="AINP5" direction="in"/>
<pin name="AINN5" direction="in"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="VCOM" direction="out"/>
<pin name="VREFP" direction="in"/>
<pin name="VREFN" direction="in"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="AINP4" direction="in"/>
<pin name="AINN4" direction="in"/>
<pin name="AINP3" direction="in"/>
<pin name="AINN3" direction="in"/>
</symbol>
<symbol name="ADS1271">
<pin name="AINP" direction="in"/>
<pin name="AINN" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="AVDD" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="FORMAT" direction="in"/>
<pin name="!SYNC!/!PDWN" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT" direction="out"/>
<pin name="!DRDY!/FSYNC"/>
<pin name="SCLK" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="DVDD" direction="in"/>
<pin name="DGND" direction="in"/>
<pin name="VREFN" direction="in"/>
<pin name="VREFP" direction="in"/>
</symbol>
<symbol name="ISO1050">
<pin name="RXD" direction="in"/>
<pin name="TXD" direction="in"/>
<pin name="CANH" direction="in"/>
<pin name="CANL" direction="in"/>
<pin name="GND1" direction="in"/>
<pin name="GND2" direction="in"/>
<pin name="VCC1" direction="in"/>
<pin name="VCC2" direction="in"/>
</symbol>
<symbol name="ADS1210">
<pin name="AINP" direction="in"/>
<pin name="AINN" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="VBIAS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="!DSYNC" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="SDOUT" direction="out"/>
<pin name="!DRDY" direction="out"/>
<pin name="MODE" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="REFOUT" direction="out"/>
<pin name="REFIN" direction="in"/>
</symbol>
<symbol name="ADS1211">
<pin name="AIN3N" direction="in"/>
<pin name="AIN2P" direction="in"/>
<pin name="AIN2N" direction="in"/>
<pin name="AIN1P" direction="in"/>
<pin name="AIN1N" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="VBIAS" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="!DSYNC" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="SDOUT" direction="out"/>
<pin name="!DRDY" direction="in"/>
<pin name="MODE" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="REFOUT" direction="out"/>
<pin name="REFIN" direction="in"/>
<pin name="AIN4P" direction="in"/>
<pin name="AIN4N" direction="in"/>
<pin name="AIN3P" direction="in"/>
</symbol>
<symbol name="ADS1211E">
<pin name="AIN3N" direction="in"/>
<pin name="AIN2P" direction="in"/>
<pin name="AIN2N" direction="in"/>
<pin name="AIN1P" direction="in"/>
<pin name="AIN1N" direction="in"/>
<pin name="AGND" direction="pwr"/>
<pin name="VBIAS" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="!CS" direction="in"/>
<pin name="!DSYNC" direction="in"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="SCLK"/>
<pin name="SDIO"/>
<pin name="SDOUT" direction="out"/>
<pin name="!DRDY" direction="out"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="MODE" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="REFOUT" direction="out"/>
<pin name="REFIN" direction="in"/>
<pin name="AIN4P" direction="in"/>
<pin name="AIN4N" direction="in"/>
<pin name="AIN3P" direction="in"/>
</symbol>
<symbol name="OMAP-L137_A">
<pin name="ACLKR0/ECAP1/APWM1/GP215"/>
<pin name="ACLKR1/ECAP2/APWM2/GP412"/>
<pin name="ACLKX0/ECAP0/APWM0/GP212"/>
<pin name="ACLKX1/EPWM0A/GP315"/>
<pin name="AFSR0/GP312"/>
<pin name="AFSR1/GP413"/>
<pin name="AFSX0/GP213/BOOT10"/>
<pin name="AFSX1/EPWMSYNCI/EPWMSYNCO/GP410"/>
<pin name="AHCLKR0/RMII_MHZ50CLK/GP214/BOOT11"/>
<pin name="AHCLKR1/GP411"/>
<pin name="AHCLKX0/AHCLKX2/USBREFCLKIN/GP211"/>
<pin name="AHCLKX1/EPWM0B/GP314"/>
<pin name="AMUTE0/!RESETOUT"/>
<pin name="AMUTE1/EPWMTZ/GP414"/>
<pin name="AXR00/RMII_TXD0/AFSR2/GP30"/>
<pin name="AXR01/RMII_TXD1/ACLKX2/GP31"/>
<pin name="AXR02/RMII_TXEN/AXR23/GP32"/>
<pin name="AXR03/RMII_CRSDV/AXR22/GP33"/>
<pin name="AXR04/RMII_RXD0/AXR21/GP34"/>
<pin name="AXR05/RMII_RXD1/AFSX2/GP35"/>
<pin name="AXR06/RMII_RXER/ACLKR2/GP36"/>
<pin name="AXR07/MDIOCLK/GP37"/>
<pin name="AXR08/MDIOD/GP38"/>
<pin name="AXR09/UART1RXD/GP39"/>
<pin name="AXR010/UART1TXD/GP310"/>
<pin name="AXR10/GP40"/>
<pin name="AXR011/AXR20/GP311"/>
<pin name="AXR11/GP41"/>
<pin name="AXR12/GP42"/>
<pin name="AXR13/EQEP1A/GP43"/>
<pin name="AXR14/EQEP1B/GP44"/>
<pin name="AXR15/EPWM2B/GP45"/>
<pin name="AXR16/EPWM2A/GP46"/>
<pin name="AXR17/EPWM1B/GP47"/>
<pin name="AXR18/EPWM1A/GP48"/>
<pin name="AXR19/GP49"/>
<pin name="AXR110/GP510"/>
<pin name="AXR111/GP511"/>
</symbol>
<symbol name="OMAP-L137_B">
<pin name="!EMA_CAS!/!EMA_CS4!/GP21"/>
<pin name="!EMA_CS0!/!UHPIHAS!/GP24"/>
<pin name="!EMA_CS2!/!UHPIHCS!/GP25/BOOT15"/>
<pin name="!EMA_CS3!/AMUTE2/GP26"/>
<pin name="!EMA_OE!/!UHPIHDS1!/AXR013/GP27"/>
<pin name="!EMA_RAS!/!EMA_CS5!/GP22"/>
<pin name="!EMA_WE!/UHPIHR!W!/AXR012/GP23/BOOT14"/>
<pin name="!EMA_WEDQM0!/!UHPIHINT!/AXR015/GP29"/>
<pin name="!EMA_WEDQM1!/!UHPIHDS2!/AXR014/GP28"/>
<pin name="EMA_A0/LCDD7/GP10"/>
<pin name="EMA_A1/MMCSDCLK/UHPIHCNTL0/GP11"/>
<pin name="EMA_A2/MMCSDCMD/UHPIHCNTL1/GP12"/>
<pin name="EMA_A3/LCDD6/GP13"/>
<pin name="EMA_A4/LCDD3/GP14"/>
<pin name="EMA_A5/LCDD2/GP15"/>
<pin name="EMA_A6/LCDD1/GP16"/>
<pin name="EMA_A7/LCDD0/GP17"/>
<pin name="EMA_A8/LCDPCLK/GP18"/>
<pin name="EMA_A9/LCDHSYNC/GP19"/>
<pin name="EMA_A10/LCDVSYNC/GP110"/>
<pin name="EMA_A11/!LCDACENBCS!/GP111"/>
<pin name="EMA_A12/LCDMCLK/GP112"/>
<pin name="EMA_BA0/LCDD4/GP114"/>
<pin name="EMA_BA1/LCDD5/UHPIHHWIL/GP113"/>
<pin name="EMA_CLK/OBSCLK/AHCLKR2/GP115"/>
<pin name="EMA_D0/MMCSDDAT0/UHPIHD0/GP00/BOOT12"/>
<pin name="EMA_D1/MMCSDDAT1/UHPIHD1/GP01"/>
<pin name="EMA_D2/MMCSDDAT2/UHPIHD2/GP02"/>
<pin name="EMA_D3/MMCSDDAT3/UHPIHD3/GP03"/>
<pin name="EMA_D4/MMCSDDAT4/UHPIHD4/GP04"/>
<pin name="EMA_D5/MMCSDDAT5/UHPIHD5/GP05"/>
<pin name="EMA_D6/MMCSDDAT6/UHPIHD6/GP06"/>
<pin name="EMA_D7/MMCSDDAT7/UHPIHD7/GP07/BOOT13"/>
<pin name="EMA_D8/UHPIHD8/LCDD8/GP08"/>
<pin name="EMA_D9/UHPIHD9/LCDD9/GP09"/>
<pin name="EMA_D10/UHPIHD10/LCDD10/GP010"/>
<pin name="EMA_D11/UHPIHD11/LCDD11/GP011"/>
<pin name="EMA_D12/UHPIHD12/LCDD12/GP012"/>
<pin name="EMA_D13/UHPIHD13/LCDD13/GP013"/>
<pin name="EMA_D14/UHPIHD14/LCDD14/GP014"/>
<pin name="EMA_D15/UHPIHD15/LCDD15/GP015"/>
<pin name="EMA_SDCKE/GP20"/>
<pin name="EMA_WAIT0/!UHPIHRDY!/GP210"/>
</symbol>
<symbol name="OMAP-L137_C">
<pin name="!EMB_CAS"/>
<pin name="!EMB_CS0"/>
<pin name="!EMB_RAS"/>
<pin name="!EMB_WE"/>
<pin name="!EMB_WEDQM0!/GP515"/>
<pin name="!EMB_WEDQM1!/GP514"/>
<pin name="!EMB_WEDQM2!"/>
<pin name="!EMB_WEDQM3!"/>
<pin name="EMB_A0/GP72"/>
<pin name="EMB_A1/GP73"/>
<pin name="EMB_A2/GP74"/>
<pin name="EMB_A3/GP75"/>
<pin name="EMB_A4/GP76"/>
<pin name="EMB_A5/GP77"/>
<pin name="EMB_A6/GP78"/>
<pin name="EMB_A7/GP79"/>
<pin name="EMB_A8/GP710"/>
<pin name="EMB_A9/GP711"/>
<pin name="EMB_A10/GP712"/>
<pin name="EMB_A11/GP713"/>
<pin name="EMB_A12/GP313"/>
<pin name="EMB_BA0/GP71"/>
<pin name="EMB_BA1/GP70"/>
<pin name="EMB_CLK"/>
<pin name="EMB_D0/GP60"/>
<pin name="EMB_D1/GP61"/>
<pin name="EMB_D2/GP62"/>
<pin name="EMB_D3/GP63"/>
<pin name="EMB_D4/GP64"/>
<pin name="EMB_D5/GP65"/>
<pin name="EMB_D6/GP66"/>
<pin name="EMB_D7/GP67"/>
<pin name="EMB_D8/GP68"/>
<pin name="EMB_D9/GP69"/>
<pin name="EMB_D10/GP610"/>
<pin name="EMB_D11/GP611"/>
<pin name="EMB_D12/GP612"/>
<pin name="EMB_D13/GP613"/>
<pin name="EMB_D14/GP614"/>
<pin name="EMB_D15/GP615"/>
<pin name="EMB_D16"/>
<pin name="EMB_D17"/>
<pin name="EMB_D18"/>
<pin name="EMB_D19"/>
<pin name="EMB_D20"/>
<pin name="EMB_D21"/>
<pin name="EMB_D22"/>
<pin name="EMB_D23"/>
<pin name="EMB_D24"/>
<pin name="EMB_D25"/>
<pin name="EMB_D26"/>
<pin name="EMB_D27"/>
<pin name="EMB_D28"/>
<pin name="EMB_D29"/>
<pin name="EMB_D30"/>
<pin name="EMB_D31"/>
<pin name="EMB_SDCKE"/>
</symbol>
<symbol name="OMAP-L137_D">
<pin name="!RESET" direction="in"/>
<pin name="!SPI0_ENA!/!UART0CTS!/EQEP0A/GP53/BOOT3"/>
<pin name="!SPI0_SCS0!/!UART0RTS!/EQEP0B/GP54/BOOT4"/>
<pin name="!SPI1_ENA!/UART2RXD/GP512"/>
<pin name="!SPI1_SCS0!/UART2TXD/GP513"/>
<pin name="!TRST" direction="in"/>
<pin name="EMU0/GP715"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="OSCIN" direction="pas"/>
<pin name="OSCOUT" direction="pas"/>
<pin name="OSCVSS" direction="pwr"/>
<pin name="PLL0_VDDA" direction="pwr"/>
<pin name="PLL0_VSSA" direction="pwr"/>
<pin name="RSV1" direction="pas"/>
<pin name="RSV2" direction="pas"/>
<pin name="RTC/XI" direction="pas"/>
<pin name="RTC/XO" direction="pas"/>
<pin name="RTCK" direction="pas"/>
<pin name="RTC_CVDD" direction="pwr"/>
<pin name="RTC_VSS" direction="pwr"/>
<pin name="SPI0_CLK/EQEP1I/GP52/BOOT2"/>
<pin name="SPI0_SIMO0/EQEP0S/GP51/BOOT1"/>
<pin name="SPI0_SOMI0/EQEP0I/GP50/BOOT0"/>
<pin name="SPI1_CLK/EQEP1S/GP57/BOOT7"/>
<pin name="SPI1_SIMO0/I2C1SDA/GP56/BOOT6"/>
<pin name="SPI1_SOMI0/I2C1SCL/GP55/BOOT5"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="UART0RXD/I2C0SDA/TM64P0IN12/GP58/BOOT8"/>
<pin name="UART0TXD/I2C0SCL/TM64P0OUT12/GP59/BOOT9"/>
<pin name="USB0/DM" direction="pas"/>
<pin name="USB0/DP" direction="pas"/>
<pin name="USB0/ID" direction="pas"/>
<pin name="USB0/VBUS" direction="pas"/>
<pin name="USB0DRVVBUS/GP415"/>
<pin name="USB1/DM" direction="pas"/>
<pin name="USB1/DP" direction="pas"/>
</symbol>
<symbol name="OMAP-L137_P">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="VDD@31" direction="pwr"/>
<pin name="VDD@32" direction="pwr"/>
<pin name="VDD@33" direction="pwr"/>
<pin name="VDD@34" direction="pwr"/>
<pin name="VDD@35" direction="pwr"/>
<pin name="VDD@36" direction="pwr"/>
<pin name="VDD@37" direction="pwr"/>
<pin name="VDD@38" direction="pwr"/>
<pin name="VDD@39" direction="pwr"/>
<pin name="VDD@40" direction="pwr"/>
<pin name="VDD@41" direction="pwr"/>
<pin name="VDD@42" direction="pwr"/>
<pin name="VDD@43" direction="pwr"/>
<pin name="VDD@45" direction="pwr"/>
<pin name="VDD@46" direction="pwr"/>
<pin name="VDD@47" direction="pwr"/>
<pin name="VDD@48" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
</symbol>
<symbol name="TMS320C64X_DSP-A">
<pin name="AARDY" direction="in"/>
<pin name="ABE_Z3" direction="out"/>
<pin name="ABE_Z4" direction="out"/>
<pin name="ABE_Z5" direction="out"/>
<pin name="ABE_Z6" direction="out"/>
<pin name="ABUSREQ" direction="out"/>
<pin name="ACE_Z3" direction="out"/>
<pin name="ACE_Z4" direction="out"/>
<pin name="ACE_Z5" direction="out"/>
<pin name="ACE_Z6" direction="out"/>
<pin name="ACLKR0"/>
<pin name="ACLKX0"/>
<pin name="AEA22"/>
<pin name="AEA23"/>
<pin name="AEA24"/>
<pin name="AEA25"/>
<pin name="AEA26"/>
<pin name="AEA27"/>
<pin name="AEA28"/>
<pin name="AEA29"/>
<pin name="AEA30"/>
<pin name="AEA31"/>
<pin name="AEA32"/>
<pin name="AEA33"/>
<pin name="AEA34"/>
<pin name="AEA35"/>
<pin name="AEA36"/>
<pin name="AEA37"/>
<pin name="AEA38"/>
<pin name="AEA39"/>
<pin name="AEA40"/>
<pin name="AEA41"/>
<pin name="AECLKIN" direction="in"/>
<pin name="AECLKOUT1" direction="out"/>
<pin name="AECLKOUT2" direction="out"/>
<pin name="AED31"/>
<pin name="AED32"/>
<pin name="AED33"/>
<pin name="AED34"/>
<pin name="AED35"/>
<pin name="AED36"/>
<pin name="AED37"/>
<pin name="AED38"/>
<pin name="AED39"/>
<pin name="AED40"/>
<pin name="AED41"/>
<pin name="AED42"/>
<pin name="AED43"/>
<pin name="AED44"/>
<pin name="AED45"/>
<pin name="AED46"/>
<pin name="AED47"/>
<pin name="AED48"/>
<pin name="AED49"/>
<pin name="AED50"/>
<pin name="AED51"/>
<pin name="AED52"/>
<pin name="AED53"/>
<pin name="AED54"/>
<pin name="AED55"/>
<pin name="AED56"/>
<pin name="AED57"/>
<pin name="AED58"/>
<pin name="AED59"/>
<pin name="AED60"/>
<pin name="AED61"/>
<pin name="AED62"/>
<pin name="AFSR0"/>
<pin name="AFSX0"/>
<pin name="AHCLKR0"/>
<pin name="AHCLKX0"/>
<pin name="AHOLDA_Z" direction="out"/>
<pin name="AHOLD_Z" direction="in"/>
<pin name="AMUTE0"/>
<pin name="AMUTEIN0" direction="in"/>
<pin name="APDTD_Z" direction="out"/>
<pin name="ASDCAS_Z" direction="out"/>
<pin name="ASDCKE" direction="out"/>
<pin name="ASDRAS_Z" direction="out"/>
<pin name="ASDWE_Z" direction="out"/>
<pin name="ASOE3_Z" direction="out"/>
<pin name="AXR05"/>
<pin name="AXR06"/>
<pin name="AXR07"/>
<pin name="AXR08"/>
<pin name="AXR09"/>
<pin name="AXR010"/>
</symbol>
<symbol name="TMS320C64X_DSP-B">
<pin name="CLKIN" direction="in"/>
<pin name="CLKINSEL" direction="in"/>
<pin name="CLKMODE3" direction="in"/>
<pin name="CLKMODE4" direction="in"/>
<pin name="CLKMODE5" direction="in"/>
<pin name="CLKMODE6" direction="in"/>
<pin name="CLKOUT4"/>
<pin name="CLKOUT6"/>
<pin name="CLKR0"/>
<pin name="CLKR1"/>
<pin name="CLKS0" direction="in"/>
<pin name="CLKS1" direction="in"/>
<pin name="CLKX0"/>
<pin name="CLKX1"/>
<pin name="DR0" direction="in"/>
<pin name="DR1" direction="in"/>
<pin name="DX0"/>
<pin name="DX1" direction="out"/>
<pin name="EMU0"/>
<pin name="EMU1" direction="in"/>
<pin name="EMU2"/>
<pin name="EMU3"/>
<pin name="EMU4"/>
<pin name="EMU5"/>
<pin name="EMU6"/>
<pin name="EMU7"/>
<pin name="EMU8"/>
<pin name="EMU9"/>
<pin name="EMU10"/>
<pin name="EMU11"/>
<pin name="EXT_INT4_Z"/>
<pin name="EXT_INT5_Z"/>
<pin name="EXT_INT6_Z"/>
<pin name="EXT_INT7_Z"/>
<pin name="RSV01" direction="pas"/>
<pin name="RSV02" direction="pas"/>
<pin name="RSV03" direction="pas"/>
<pin name="RSV04" direction="pas"/>
<pin name="RSV05" direction="out"/>
<pin name="RSV06" direction="in"/>
<pin name="RSV07" direction="pas"/>
<pin name="RSV08" direction="pas"/>
</symbol>
<symbol name="TMS320C64X_DSP-C">
<pin name="FSR0"/>
<pin name="FSR1"/>
<pin name="FSX0"/>
<pin name="FSX1"/>
<pin name="GP0_00"/>
<pin name="GP0_03"/>
<pin name="HAS_Z" direction="in"/>
<pin name="HCNTL1" direction="in"/>
<pin name="HCNTL2" direction="in"/>
<pin name="HCS_Z" direction="in"/>
<pin name="HD31"/>
<pin name="HD32"/>
<pin name="HD33"/>
<pin name="HD34"/>
<pin name="HD35"/>
<pin name="HD36"/>
<pin name="HD37"/>
<pin name="HD38"/>
<pin name="HD39"/>
<pin name="HD40"/>
<pin name="HD41"/>
<pin name="HD42"/>
<pin name="HD43"/>
<pin name="HD44"/>
<pin name="HD45"/>
<pin name="HD46"/>
<pin name="HD47"/>
<pin name="HD48"/>
<pin name="HD49"/>
<pin name="HD50"/>
<pin name="HD51"/>
<pin name="HD52"/>
<pin name="HD53"/>
<pin name="HD54"/>
<pin name="HD55"/>
<pin name="HD56"/>
<pin name="HD57"/>
<pin name="HD58"/>
<pin name="HD59"/>
<pin name="HD60"/>
<pin name="HD61"/>
<pin name="HD62"/>
<pin name="HDS1_Z" direction="in"/>
<pin name="HDS2_Z" direction="in"/>
<pin name="HHWIL" direction="in"/>
<pin name="HINT_Z"/>
<pin name="HRDY_Z"/>
<pin name="HRW" direction="in"/>
<pin name="NMI" direction="in"/>
<pin name="OSCIN" direction="pas"/>
<pin name="OSCOUT" direction="pas"/>
<pin name="OSCVDD" direction="pas"/>
<pin name="OSCVSS" direction="pas"/>
<pin name="OSC_DIS" direction="in"/>
<pin name="PLLV" direction="pas"/>
<pin name="RESET_Z" direction="in"/>
<pin name="SCL0"/>
<pin name="SCL1"/>
<pin name="SDA0"/>
<pin name="SDA1"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TINP0" direction="in"/>
<pin name="TINP1" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TOUT0"/>
<pin name="TOUT1"/>
<pin name="TRST_Z" direction="in"/>
</symbol>
<symbol name="TMS320C64X_DSP-P">
<pin name="CVDD@21" direction="pas"/>
<pin name="CVDD@22" direction="pas"/>
<pin name="CVDD@23" direction="pas"/>
<pin name="CVDD@24" direction="pas"/>
<pin name="CVDD@25" direction="pas"/>
<pin name="CVDD@26" direction="pas"/>
<pin name="CVDD@27" direction="pas"/>
<pin name="CVDD@28" direction="pas"/>
<pin name="CVDD@29" direction="pas"/>
<pin name="CVDD@30" direction="pas"/>
<pin name="CVDD@31" direction="pas"/>
<pin name="CVDD@32" direction="pas"/>
<pin name="CVDD@33" direction="pas"/>
<pin name="CVDD@34" direction="pas"/>
<pin name="CVDD@35" direction="pas"/>
<pin name="CVDD@36" direction="pas"/>
<pin name="CVDD@37" direction="pas"/>
<pin name="CVDD@38" direction="pas"/>
<pin name="CVDD@39" direction="pas"/>
<pin name="CVDD@40" direction="pas"/>
<pin name="CVDD@41" direction="pas"/>
<pin name="CVDD@42" direction="pas"/>
<pin name="DVDD@23" direction="pas"/>
<pin name="DVDD@24" direction="pas"/>
<pin name="DVDD@25" direction="pas"/>
<pin name="DVDD@26" direction="pas"/>
<pin name="DVDD@27" direction="pas"/>
<pin name="DVDD@28" direction="pas"/>
<pin name="DVDD@29" direction="pas"/>
<pin name="DVDD@30" direction="pas"/>
<pin name="DVDD@31" direction="pas"/>
<pin name="DVDD@32" direction="pas"/>
<pin name="DVDD@33" direction="pas"/>
<pin name="DVDD@34" direction="pas"/>
<pin name="DVDD@35" direction="pas"/>
<pin name="DVDD@36" direction="pas"/>
<pin name="DVDD@37" direction="pas"/>
<pin name="DVDD@38" direction="pas"/>
<pin name="DVDD@39" direction="pas"/>
<pin name="DVDD@40" direction="pas"/>
<pin name="DVDD@41" direction="pas"/>
<pin name="DVDD@42" direction="pas"/>
<pin name="DVDD@43" direction="pas"/>
<pin name="DVDD@44" direction="pas"/>
<pin name="DVDD@45" direction="pas"/>
<pin name="DVDD@46" direction="pas"/>
<pin name="VSS@43" direction="pas"/>
<pin name="VSS@44" direction="pas"/>
<pin name="VSS@45" direction="pas"/>
<pin name="VSS@46" direction="pas"/>
<pin name="VSS@47" direction="pas"/>
<pin name="VSS@48" direction="pas"/>
<pin name="VSS@49" direction="pas"/>
<pin name="VSS@50" direction="pas"/>
<pin name="VSS@51" direction="pas"/>
<pin name="VSS@52" direction="pas"/>
<pin name="VSS@53" direction="pas"/>
<pin name="VSS@54" direction="pas"/>
<pin name="VSS@55" direction="pas"/>
<pin name="VSS@56" direction="pas"/>
<pin name="VSS@57" direction="pas"/>
<pin name="VSS@58" direction="pas"/>
<pin name="VSS@59" direction="pas"/>
<pin name="VSS@60" direction="pas"/>
<pin name="VSS@61" direction="pas"/>
<pin name="VSS@62" direction="pas"/>
<pin name="VSS@63" direction="pas"/>
<pin name="VSS@64" direction="pas"/>
<pin name="VSS@65" direction="pas"/>
<pin name="VSS@66" direction="pas"/>
<pin name="VSS@67" direction="pas"/>
<pin name="VSS@68" direction="pas"/>
<pin name="VSS@69" direction="pas"/>
<pin name="VSS@70" direction="pas"/>
<pin name="VSS@71" direction="pas"/>
<pin name="VSS@72" direction="pas"/>
<pin name="VSS@73" direction="pas"/>
<pin name="VSS@74" direction="pas"/>
<pin name="VSS@75" direction="pas"/>
<pin name="VSS@76" direction="pas"/>
<pin name="VSS@77" direction="pas"/>
<pin name="VSS@78" direction="pas"/>
<pin name="VSS@79" direction="pas"/>
<pin name="VSS@80" direction="pas"/>
<pin name="VSS@81" direction="pas"/>
<pin name="VSS@82" direction="pas"/>
<pin name="VSS@83" direction="pas"/>
<pin name="VSS@84" direction="pas"/>
<pin name="VSS@85" direction="pas"/>
<pin name="VSS@86" direction="pas"/>
</symbol>
<symbol name="TMS320C6474-A">
<pin name="AIFRXN0" direction="pas"/>
<pin name="AIFRXN1" direction="pas"/>
<pin name="AIFRXN2" direction="pas"/>
<pin name="AIFRXN3" direction="pas"/>
<pin name="AIFRXN4" direction="pas"/>
<pin name="AIFRXN5" direction="pas"/>
<pin name="AIFRXP0" direction="pas"/>
<pin name="AIFRXP1" direction="pas"/>
<pin name="AIFRXP2" direction="pas"/>
<pin name="AIFRXP3" direction="pas"/>
<pin name="AIFRXP4" direction="pas"/>
<pin name="AIFRXP5" direction="pas"/>
<pin name="AIFTXN0" direction="pas"/>
<pin name="AIFTXN1" direction="pas"/>
<pin name="AIFTXN2" direction="pas"/>
<pin name="AIFTXN3" direction="pas"/>
<pin name="AIFTXN4" direction="pas"/>
<pin name="AIFTXN5" direction="pas"/>
<pin name="AIFTXP0" direction="pas"/>
<pin name="AIFTXP1" direction="pas"/>
<pin name="AIFTXP2" direction="pas"/>
<pin name="AIFTXP3" direction="pas"/>
<pin name="AIFTXP4" direction="pas"/>
<pin name="AIFTXP5" direction="pas"/>
<pin name="ALTCORECLKN" direction="pas"/>
<pin name="ALTCORECLKP" direction="pas"/>
<pin name="ALTFSYNCCLK" direction="pas"/>
<pin name="ALTFSYNCPULSE" direction="pas"/>
</symbol>
<symbol name="TMS320C6474-B">
<pin name="CLKR0" direction="pas"/>
<pin name="CLKR1" direction="pas"/>
<pin name="CLKS0" direction="pas"/>
<pin name="CLKS1" direction="pas"/>
<pin name="CLKX0" direction="pas"/>
<pin name="CLKX1" direction="pas"/>
<pin name="CORECLKSEL" direction="pas"/>
<pin name="DDRA00" direction="pas"/>
<pin name="DDRA01" direction="pas"/>
<pin name="DDRA02" direction="pas"/>
<pin name="DDRA03" direction="pas"/>
<pin name="DDRA04" direction="pas"/>
<pin name="DDRA05" direction="pas"/>
<pin name="DDRA06" direction="pas"/>
<pin name="DDRA07" direction="pas"/>
<pin name="DDRA08" direction="pas"/>
<pin name="DDRA09" direction="pas"/>
<pin name="DDRA10" direction="pas"/>
<pin name="DDRA11" direction="pas"/>
<pin name="DDRA12" direction="pas"/>
<pin name="DDRA13" direction="pas"/>
<pin name="DDRBA0" direction="pas"/>
<pin name="DDRBA1" direction="pas"/>
<pin name="DDRBA2" direction="pas"/>
<pin name="DDRCASZ" direction="pas"/>
<pin name="DDRCEZ" direction="pas"/>
<pin name="DDRCKE" direction="pas"/>
<pin name="DDRCLKOUTN0" direction="pas"/>
<pin name="DDRCLKOUTN1" direction="pas"/>
<pin name="DDRCLKOUTP0" direction="pas"/>
<pin name="DDRCLKOUTP1" direction="pas"/>
<pin name="DDRD00" direction="pas"/>
<pin name="DDRD01" direction="pas"/>
<pin name="DDRD02" direction="pas"/>
<pin name="DDRD03" direction="pas"/>
<pin name="DDRD04" direction="pas"/>
<pin name="DDRD05" direction="pas"/>
<pin name="DDRD06" direction="pas"/>
<pin name="DDRD07" direction="pas"/>
<pin name="DDRD08" direction="pas"/>
<pin name="DDRD09" direction="pas"/>
<pin name="DDRD10" direction="pas"/>
<pin name="DDRD11" direction="pas"/>
<pin name="DDRD12" direction="pas"/>
<pin name="DDRD13" direction="pas"/>
<pin name="DDRD14" direction="pas"/>
<pin name="DDRD15" direction="pas"/>
<pin name="DDRD16" direction="pas"/>
<pin name="DDRD17" direction="pas"/>
<pin name="DDRD18" direction="pas"/>
<pin name="DDRD19" direction="pas"/>
<pin name="DDRD20" direction="pas"/>
<pin name="DDRD21" direction="pas"/>
<pin name="DDRD22" direction="pas"/>
<pin name="DDRD23" direction="pas"/>
<pin name="DDRD24" direction="pas"/>
<pin name="DDRD25" direction="pas"/>
<pin name="DDRD26" direction="pas"/>
<pin name="DDRD27" direction="pas"/>
<pin name="DDRD28" direction="pas"/>
<pin name="DDRD29" direction="pas"/>
<pin name="DDRD30" direction="pas"/>
<pin name="DDRD31" direction="pas"/>
<pin name="DDRDQM0" direction="pas"/>
<pin name="DDRDQM1" direction="pas"/>
<pin name="DDRDQM2" direction="pas"/>
<pin name="DDRDQM3" direction="pas"/>
<pin name="DDRDQS0N" direction="pas"/>
<pin name="DDRDQS0P" direction="pas"/>
<pin name="DDRDQS1N" direction="pas"/>
<pin name="DDRDQS1P" direction="pas"/>
<pin name="DDRDQS2N" direction="pas"/>
<pin name="DDRDQS2P" direction="pas"/>
<pin name="DDRDQS3N" direction="pas"/>
<pin name="DDRDQS3P" direction="pas"/>
<pin name="DDRODT" direction="pas"/>
<pin name="DDRRASZ" direction="pas"/>
<pin name="DDRRCVENIN0" direction="pas"/>
<pin name="DDRRCVENIN1" direction="pas"/>
<pin name="DDRRCVENOUT0" direction="pas"/>
<pin name="DDRRCVENOUT1" direction="pas"/>
<pin name="DDRREFCLKN" direction="pas"/>
<pin name="DDRREFCLKP" direction="pas"/>
<pin name="DDRSLRATE" direction="pas"/>
<pin name="DDRWEZ" direction="pas"/>
<pin name="DR0" direction="pas"/>
<pin name="DR1" direction="pas"/>
<pin name="DX0" direction="pas"/>
<pin name="DX1" direction="pas"/>
</symbol>
<symbol name="TMS320C6474-C">
<pin name="EMU00" direction="pas"/>
<pin name="EMU01" direction="pas"/>
<pin name="EMU02" direction="pas"/>
<pin name="EMU03" direction="pas"/>
<pin name="EMU04" direction="pas"/>
<pin name="EMU05" direction="pas"/>
<pin name="EMU06" direction="pas"/>
<pin name="EMU07" direction="pas"/>
<pin name="EMU08" direction="pas"/>
<pin name="EMU09" direction="pas"/>
<pin name="EMU10" direction="pas"/>
<pin name="EMU11" direction="pas"/>
<pin name="EMU12" direction="pas"/>
<pin name="EMU13" direction="pas"/>
<pin name="EMU14" direction="pas"/>
<pin name="EMU15" direction="pas"/>
<pin name="EMU16" direction="pas"/>
<pin name="EMU17" direction="pas"/>
<pin name="EMU18" direction="pas"/>
<pin name="FRAMEBURSTN" direction="pas"/>
<pin name="FRAMEBURSTP" direction="pas"/>
<pin name="FSR0" direction="pas"/>
<pin name="FSR1" direction="pas"/>
<pin name="FSX0" direction="pas"/>
<pin name="FSX1" direction="pas"/>
<pin name="FSYNCCLKN" direction="pas"/>
<pin name="FSYNCCLKP" direction="pas"/>
<pin name="GP00" direction="pas"/>
<pin name="GP01" direction="pas"/>
<pin name="GP02" direction="pas"/>
<pin name="GP03" direction="pas"/>
<pin name="GP04" direction="pas"/>
<pin name="GP05" direction="pas"/>
<pin name="GP06" direction="pas"/>
<pin name="GP07" direction="pas"/>
<pin name="GP08" direction="pas"/>
<pin name="GP09" direction="pas"/>
<pin name="GP10" direction="pas"/>
<pin name="GP11" direction="pas"/>
<pin name="GP12" direction="pas"/>
<pin name="GP13" direction="pas"/>
<pin name="GP14" direction="pas"/>
<pin name="GP15" direction="pas"/>
<pin name="MDCLK" direction="pas"/>
<pin name="MDIO" direction="pas"/>
<pin name="NMI0" direction="pas"/>
<pin name="NMI1" direction="pas"/>
<pin name="NMI2" direction="pas"/>
</symbol>
<symbol name="TMS320C6474-D">
<pin name="PORZ" direction="pas"/>
<pin name="RESETSTATZ" direction="pas"/>
<pin name="RIORXN0" direction="pas"/>
<pin name="RIORXN1" direction="pas"/>
<pin name="RIORXP0" direction="pas"/>
<pin name="RIORXP1" direction="pas"/>
<pin name="RIOSGMIICLKN" direction="pas"/>
<pin name="RIOSGMIICLKP" direction="pas"/>
<pin name="RIOTXN0" direction="pas"/>
<pin name="RIOTXN1" direction="pas"/>
<pin name="RIOTXP0" direction="pas"/>
<pin name="RIOTXP1" direction="pas"/>
<pin name="RSV01" direction="pas"/>
<pin name="RSV02" direction="pas"/>
<pin name="RSV03" direction="pas"/>
<pin name="RSV04" direction="pas"/>
<pin name="RSV05" direction="pas"/>
<pin name="RSV06" direction="pas"/>
<pin name="RSV07" direction="pas"/>
<pin name="RSV08" direction="pas"/>
<pin name="RSV09" direction="pas"/>
<pin name="RSV10" direction="pas"/>
<pin name="RSV11" direction="pas"/>
<pin name="RSV12" direction="pas"/>
<pin name="RSV13" direction="pas"/>
<pin name="RSV14" direction="pas"/>
<pin name="RSV15" direction="pas"/>
<pin name="RSV16" direction="pas"/>
<pin name="RSV17" direction="pas"/>
<pin name="RSV18" direction="pas"/>
<pin name="RSV19" direction="pas"/>
<pin name="RSV20" direction="pas"/>
<pin name="RSV21" direction="pas"/>
<pin name="RSV22" direction="pas"/>
<pin name="RSV23" direction="pas"/>
<pin name="RSV24" direction="pas"/>
<pin name="RSV25" direction="pas"/>
<pin name="RSV26" direction="pas"/>
<pin name="RSV27" direction="pas"/>
<pin name="RSV28" direction="pas"/>
<pin name="RSV29" direction="pas"/>
<pin name="SCL" direction="pas"/>
<pin name="SDA" direction="pas"/>
<pin name="SGMIIRXN" direction="pas"/>
<pin name="SGMIIRXP" direction="pas"/>
<pin name="SGMIITXN" direction="pas"/>
<pin name="SGMIITXP" direction="pas"/>
<pin name="SMFRAMECLK" direction="pas"/>
<pin name="SYSCLKN" direction="pas"/>
<pin name="SYSCLKOUT" direction="pas"/>
<pin name="SYSCLKP" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="TIMI0" direction="pas"/>
<pin name="TIMI1" direction="pas"/>
<pin name="TIMO0" direction="pas"/>
<pin name="TIMO1" direction="pas"/>
<pin name="TMS" direction="pas"/>
<pin name="TRSTZ" direction="pas"/>
<pin name="TRT" direction="pas"/>
<pin name="TRTCLK" direction="pas"/>
<pin name="VCNTL0" direction="pas"/>
<pin name="VCNTL1" direction="pas"/>
<pin name="VCNTL2" direction="pas"/>
<pin name="VCNTL3" direction="pas"/>
<pin name="VREFSSTL" direction="pas"/>
</symbol>
<symbol name="TMS320C6474-P">
<pin name="AIF_VDDA_11" direction="pas"/>
<pin name="AIF_VDDA_11@1" direction="pas"/>
<pin name="AIF_VDDA_11@2" direction="pas"/>
<pin name="AIF_VDDA_11@3" direction="pas"/>
<pin name="AIF_VDDA_11@4" direction="pas"/>
<pin name="AIF_VDDA_11@5" direction="pas"/>
<pin name="AIF_VDDA_11@6" direction="pas"/>
<pin name="AIF_VDDA_11@7" direction="pas"/>
<pin name="AIF_VDDA_11@8" direction="pas"/>
<pin name="AIF_VDDA_11@9" direction="pas"/>
<pin name="AIF_VDDA_11@10" direction="pas"/>
<pin name="AIF_VDDR_18" direction="pas"/>
<pin name="AIF_VDDR_18@1" direction="pas"/>
<pin name="AIF_VDDT_11" direction="pas"/>
<pin name="AIF_VDDT_11@1" direction="pas"/>
<pin name="AIF_VDDT_11@2" direction="pas"/>
<pin name="AIF_VDDT_11@3" direction="pas"/>
<pin name="AIF_VDDT_11@4" direction="pas"/>
<pin name="AIF_VDDT_11@5" direction="pas"/>
<pin name="AIF_VDDT_11@6" direction="pas"/>
<pin name="AVDD1_18" direction="pas"/>
<pin name="AVDD2_18" direction="pas"/>
<pin name="CVDD" direction="pas"/>
<pin name="CVDD@1" direction="pas"/>
<pin name="CVDD@2" direction="pas"/>
<pin name="CVDD@3" direction="pas"/>
<pin name="CVDD@4" direction="pas"/>
<pin name="CVDD@5" direction="pas"/>
<pin name="CVDD@6" direction="pas"/>
<pin name="CVDD@7" direction="pas"/>
<pin name="CVDD@8" direction="pas"/>
<pin name="CVDD@9" direction="pas"/>
<pin name="CVDD@10" direction="pas"/>
<pin name="CVDD@11" direction="pas"/>
<pin name="CVDD@12" direction="pas"/>
<pin name="CVDD@13" direction="pas"/>
<pin name="CVDD@14" direction="pas"/>
<pin name="CVDD@15" direction="pas"/>
<pin name="CVDD@16" direction="pas"/>
<pin name="CVDD@17" direction="pas"/>
<pin name="CVDD@18" direction="pas"/>
<pin name="CVDD@19" direction="pas"/>
<pin name="CVDD@20" direction="pas"/>
<pin name="CVDD@21" direction="pas"/>
<pin name="CVDD@22" direction="pas"/>
<pin name="CVDD@23" direction="pas"/>
<pin name="CVDD@24" direction="pas"/>
<pin name="CVDD@25" direction="pas"/>
<pin name="CVDD@26" direction="pas"/>
<pin name="CVDD@27" direction="pas"/>
<pin name="CVDD@28" direction="pas"/>
<pin name="CVDD@29" direction="pas"/>
<pin name="CVDD@30" direction="pas"/>
<pin name="CVDD@31" direction="pas"/>
<pin name="CVDD@32" direction="pas"/>
<pin name="CVDD@33" direction="pas"/>
<pin name="CVDD@34" direction="pas"/>
<pin name="CVDD@35" direction="pas"/>
<pin name="CVDD@36" direction="pas"/>
<pin name="CVDD@37" direction="pas"/>
<pin name="CVDD@38" direction="pas"/>
<pin name="CVDD@39" direction="pas"/>
<pin name="CVDD@40" direction="pas"/>
<pin name="CVDD@41" direction="pas"/>
<pin name="CVDD@42" direction="pas"/>
<pin name="CVDD@43" direction="pas"/>
<pin name="CVDD@44" direction="pas"/>
<pin name="CVDD@45" direction="pas"/>
<pin name="CVDD@46" direction="pas"/>
<pin name="CVDD@47" direction="pas"/>
<pin name="CVDD@48" direction="pas"/>
<pin name="CVDD@49" direction="pas"/>
<pin name="CVDD_MON" direction="pas"/>
<pin name="DVDD_18" direction="pas"/>
<pin name="DVDD_18@1" direction="pas"/>
<pin name="DVDD_18@2" direction="pas"/>
<pin name="DVDD_18@3" direction="pas"/>
<pin name="DVDD_18@4" direction="pas"/>
<pin name="DVDD_18@5" direction="pas"/>
<pin name="DVDD_18@6" direction="pas"/>
<pin name="DVDD_18@7" direction="pas"/>
<pin name="DVDD_18@8" direction="pas"/>
<pin name="DVDD_18@9" direction="pas"/>
<pin name="DVDD_18@10" direction="pas"/>
<pin name="DVDD_18@11" direction="pas"/>
<pin name="DVDD_18@12" direction="pas"/>
<pin name="DVDD_18@13" direction="pas"/>
<pin name="DVDD_18@14" direction="pas"/>
<pin name="DVDD_18@15" direction="pas"/>
<pin name="DVDD_18@16" direction="pas"/>
<pin name="DVDD_18@17" direction="pas"/>
<pin name="DVDD_18@18" direction="pas"/>
<pin name="DVDD_18@19" direction="pas"/>
<pin name="DVDD_18@20" direction="pas"/>
<pin name="DVDD_18@21" direction="pas"/>
<pin name="DVDD_18@22" direction="pas"/>
<pin name="DVDD_18@23" direction="pas"/>
<pin name="DVDD_18@24" direction="pas"/>
<pin name="DVDD_18@25" direction="pas"/>
<pin name="DVDD_18@26" direction="pas"/>
<pin name="DVDD_18@27" direction="pas"/>
<pin name="DVDD_18@28" direction="pas"/>
<pin name="DVDD_18@29" direction="pas"/>
<pin name="DVDD_18@30" direction="pas"/>
<pin name="DVDD_18@31" direction="pas"/>
<pin name="DVDD_18@32" direction="pas"/>
<pin name="DVDD_18@33" direction="pas"/>
<pin name="DVDD_18@34" direction="pas"/>
<pin name="DVDD_18@35" direction="pas"/>
<pin name="DVDD_18@36" direction="pas"/>
<pin name="DVDD_18@37" direction="pas"/>
<pin name="DVDD_18@38" direction="pas"/>
<pin name="DVDD_18@39" direction="pas"/>
<pin name="DVDD_18@40" direction="pas"/>
<pin name="DVDD_18@41" direction="pas"/>
<pin name="DVDD_18@42" direction="pas"/>
<pin name="DVDD_18@43" direction="pas"/>
<pin name="DVDD_18@44" direction="pas"/>
<pin name="DVDD_18@45" direction="pas"/>
<pin name="DVDD_18@46" direction="pas"/>
<pin name="DVDD_18_MON" direction="pas"/>
<pin name="SGR_VDDA_11" direction="pas"/>
<pin name="SGR_VDDA_11@1" direction="pas"/>
<pin name="SGR_VDDA_11@2" direction="pas"/>
<pin name="SGR_VDDA_11@3" direction="pas"/>
<pin name="SGR_VDDD_11" direction="pas"/>
<pin name="SGR_VDDD_11@1" direction="pas"/>
<pin name="SGR_VDDD_11@2" direction="pas"/>
<pin name="SGR_VDDD_11@3" direction="pas"/>
<pin name="SGR_VDDD_11@4" direction="pas"/>
<pin name="SGR_VDDR_18" direction="pas"/>
<pin name="SGR_VDDR_18@1" direction="pas"/>
<pin name="SGR_VDDT_11" direction="pas"/>
<pin name="SGR_VDDT_11@1" direction="pas"/>
<pin name="SGR_VDDT_11@2" direction="pas"/>
<pin name="SGR_VDDT_11@3" direction="pas"/>
<pin name="SGR_VDDT_11@4" direction="pas"/>
<pin name="SGR_VDDT_11@5" direction="pas"/>
<pin name="VSS" direction="pas"/>
<pin name="VSS@1" direction="pas"/>
<pin name="VSS@2" direction="pas"/>
<pin name="VSS@3" direction="pas"/>
<pin name="VSS@4" direction="pas"/>
<pin name="VSS@5" direction="pas"/>
<pin name="VSS@6" direction="pas"/>
<pin name="VSS@7" direction="pas"/>
<pin name="VSS@8" direction="pas"/>
<pin name="VSS@9" direction="pas"/>
<pin name="VSS@10" direction="pas"/>
<pin name="VSS@11" direction="pas"/>
<pin name="VSS@12" direction="pas"/>
<pin name="VSS@13" direction="pas"/>
<pin name="VSS@14" direction="pas"/>
<pin name="VSS@15" direction="pas"/>
<pin name="VSS@16" direction="pas"/>
<pin name="VSS@17" direction="pas"/>
<pin name="VSS@18" direction="pas"/>
<pin name="VSS@19" direction="pas"/>
<pin name="VSS@20" direction="pas"/>
<pin name="VSS@21" direction="pas"/>
<pin name="VSS@22" direction="pas"/>
<pin name="VSS@23" direction="pas"/>
<pin name="VSS@24" direction="pas"/>
<pin name="VSS@25" direction="pas"/>
<pin name="VSS@26" direction="pas"/>
<pin name="VSS@27" direction="pas"/>
<pin name="VSS@28" direction="pas"/>
<pin name="VSS@29" direction="pas"/>
<pin name="VSS@30" direction="pas"/>
<pin name="VSS@31" direction="pas"/>
<pin name="VSS@32" direction="pas"/>
<pin name="VSS@33" direction="pas"/>
<pin name="VSS@34" direction="pas"/>
<pin name="VSS@35" direction="pas"/>
<pin name="VSS@36" direction="pas"/>
<pin name="VSS@37" direction="pas"/>
<pin name="VSS@38" direction="pas"/>
<pin name="VSS@39" direction="pas"/>
<pin name="VSS@40" direction="pas"/>
<pin name="VSS@41" direction="pas"/>
<pin name="VSS@42" direction="pas"/>
<pin name="VSS@43" direction="pas"/>
<pin name="VSS@44" direction="pas"/>
<pin name="VSS@45" direction="pas"/>
<pin name="VSS@46" direction="pas"/>
<pin name="VSS@47" direction="pas"/>
<pin name="VSS@48" direction="pas"/>
<pin name="VSS@49" direction="pas"/>
<pin name="VSS@50" direction="pas"/>
<pin name="VSS@51" direction="pas"/>
<pin name="VSS@52" direction="pas"/>
<pin name="VSS@53" direction="pas"/>
<pin name="VSS@54" direction="pas"/>
<pin name="VSS@55" direction="pas"/>
<pin name="VSS@56" direction="pas"/>
<pin name="VSS@57" direction="pas"/>
<pin name="VSS@58" direction="pas"/>
<pin name="VSS@59" direction="pas"/>
<pin name="VSS@60" direction="pas"/>
<pin name="VSS@61" direction="pas"/>
<pin name="VSS@62" direction="pas"/>
<pin name="VSS@63" direction="pas"/>
<pin name="VSS@64" direction="pas"/>
<pin name="VSS@65" direction="pas"/>
<pin name="VSS@66" direction="pas"/>
<pin name="VSS@67" direction="pas"/>
<pin name="VSS@68" direction="pas"/>
<pin name="VSS@69" direction="pas"/>
<pin name="VSS@70" direction="pas"/>
<pin name="VSS@71" direction="pas"/>
<pin name="VSS@72" direction="pas"/>
<pin name="VSS@73" direction="pas"/>
<pin name="VSS@74" direction="pas"/>
<pin name="VSS@75" direction="pas"/>
<pin name="VSS@76" direction="pas"/>
<pin name="VSS@77" direction="pas"/>
<pin name="VSS@78" direction="pas"/>
<pin name="VSS@79" direction="pas"/>
<pin name="VSS@80" direction="pas"/>
<pin name="VSS@81" direction="pas"/>
<pin name="VSS@82" direction="pas"/>
<pin name="VSS@83" direction="pas"/>
<pin name="VSS@84" direction="pas"/>
<pin name="VSS@85" direction="pas"/>
<pin name="VSS@86" direction="pas"/>
<pin name="VSS@87" direction="pas"/>
<pin name="VSS@88" direction="pas"/>
<pin name="VSS@89" direction="pas"/>
<pin name="VSS@90" direction="pas"/>
<pin name="VSS@91" direction="pas"/>
<pin name="VSS@92" direction="pas"/>
<pin name="VSS@93" direction="pas"/>
<pin name="VSS@94" direction="pas"/>
<pin name="VSS@95" direction="pas"/>
<pin name="VSS@96" direction="pas"/>
<pin name="VSS@97" direction="pas"/>
<pin name="VSS@98" direction="pas"/>
<pin name="VSS@99" direction="pas"/>
<pin name="VSS@100" direction="pas"/>
<pin name="VSS@101" direction="pas"/>
<pin name="VSS@102" direction="pas"/>
<pin name="VSS@103" direction="pas"/>
<pin name="VSS@104" direction="pas"/>
<pin name="VSS@105" direction="pas"/>
<pin name="VSS@106" direction="pas"/>
<pin name="VSS@107" direction="pas"/>
<pin name="VSS@108" direction="pas"/>
<pin name="VSS@109" direction="pas"/>
<pin name="VSS@110" direction="pas"/>
<pin name="VSS@111" direction="pas"/>
<pin name="VSS@112" direction="pas"/>
<pin name="VSS@113" direction="pas"/>
<pin name="VSS@114" direction="pas"/>
<pin name="VSS@115" direction="pas"/>
<pin name="VSS@116" direction="pas"/>
<pin name="VSS@117" direction="pas"/>
<pin name="VSS@118" direction="pas"/>
<pin name="VSS@119" direction="pas"/>
<pin name="VSS@120" direction="pas"/>
<pin name="VSS@121" direction="pas"/>
<pin name="VSS@122" direction="pas"/>
<pin name="VSS@123" direction="pas"/>
<pin name="VSS@124" direction="pas"/>
<pin name="VSS@125" direction="pas"/>
<pin name="VSS@126" direction="pas"/>
<pin name="VSS@127" direction="pas"/>
<pin name="VSS@128" direction="pas"/>
<pin name="VSS@129" direction="pas"/>
<pin name="VSS@130" direction="pas"/>
<pin name="VSS@131" direction="pas"/>
<pin name="VSS@132" direction="pas"/>
<pin name="VSS@133" direction="pas"/>
<pin name="VSS@134" direction="pas"/>
<pin name="VSS@135" direction="pas"/>
<pin name="VSS@136" direction="pas"/>
<pin name="VSS@137" direction="pas"/>
<pin name="VSS@138" direction="pas"/>
<pin name="VSS@139" direction="pas"/>
<pin name="VSS@140" direction="pas"/>
<pin name="VSS@141" direction="pas"/>
<pin name="VSS@142" direction="pas"/>
<pin name="VSS@143" direction="pas"/>
<pin name="VSS@144" direction="pas"/>
<pin name="VSS@145" direction="pas"/>
<pin name="VSS@146" direction="pas"/>
<pin name="VSS@147" direction="pas"/>
<pin name="VSS@148" direction="pas"/>
<pin name="VSS@149" direction="pas"/>
<pin name="VSS@150" direction="pas"/>
<pin name="VSS@151" direction="pas"/>
<pin name="VSS@152" direction="pas"/>
<pin name="VSS@153" direction="pas"/>
<pin name="VSS@154" direction="pas"/>
<pin name="VSS@155" direction="pas"/>
<pin name="VSS@156" direction="pas"/>
<pin name="VSS@157" direction="pas"/>
<pin name="VSS@158" direction="pas"/>
<pin name="VSS@159" direction="pas"/>
<pin name="VSS@160" direction="pas"/>
<pin name="VSS@161" direction="pas"/>
<pin name="VSS@162" direction="pas"/>
<pin name="VSS@163" direction="pas"/>
<pin name="VSS@164" direction="pas"/>
<pin name="VSS@165" direction="pas"/>
<pin name="VSS@166" direction="pas"/>
<pin name="VSS@167" direction="pas"/>
<pin name="VSS@168" direction="pas"/>
<pin name="VSS@169" direction="pas"/>
<pin name="VSS@170" direction="pas"/>
<pin name="VSS@171" direction="pas"/>
<pin name="VSS@172" direction="pas"/>
<pin name="VSS@173" direction="pas"/>
<pin name="VSS@174" direction="pas"/>
<pin name="VSS@175" direction="pas"/>
<pin name="VSS@176" direction="pas"/>
<pin name="VSS@177" direction="pas"/>
<pin name="VSS@178" direction="pas"/>
<pin name="VSS@179" direction="pas"/>
<pin name="VSS@180" direction="pas"/>
<pin name="VSS@181" direction="pas"/>
<pin name="VSS@182" direction="pas"/>
<pin name="VSS@183" direction="pas"/>
<pin name="VSS@184" direction="pas"/>
<pin name="VSS@185" direction="pas"/>
<pin name="VSS@186" direction="pas"/>
<pin name="VSS@187" direction="pas"/>
<pin name="VSS@188" direction="pas"/>
<pin name="VSS@189" direction="pas"/>
<pin name="XWRSTZ" direction="pas"/>
</symbol>
<symbol name="TAS5261">
<pin name="BST_A" direction="in"/>
<pin name="GVDD_A" direction="in"/>
<pin name="!OTW" direction="in"/>
<pin name="!SD" direction="in"/>
<pin name="!RESET" direction="in"/>
<pin name="PWM_A" direction="in"/>
<pin name="OC_ADJ" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="AGND" direction="in"/>
<pin name="VREG" direction="in"/>
<pin name="M3" direction="in"/>
<pin name="M2" direction="in"/>
<pin name="M1" direction="in"/>
<pin name="PWM_B" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="GVDD_B" direction="in"/>
<pin name="BST_B" direction="in"/>
<pin name="PVDD_B@1" direction="in"/>
<pin name="PVDD_B@2" direction="in"/>
<pin name="PVDD_B@3" direction="in"/>
<pin name="PGND@1" direction="in"/>
<pin name="PGND@2" direction="in"/>
<pin name="PGND@3" direction="in"/>
<pin name="OUT_B@1" direction="in"/>
<pin name="OUT_B@2" direction="in"/>
<pin name="OUT_B@3" direction="in"/>
<pin name="OUT_A@1" direction="in"/>
<pin name="OUT_A@2" direction="in"/>
<pin name="OUT_A@3" direction="in"/>
<pin name="PVDD_A@1" direction="in"/>
<pin name="PVDD_A@2" direction="in"/>
<pin name="PVDD_A@3" direction="in"/>
<pin name="PGND@4" direction="in"/>
<pin name="PGND@5" direction="in"/>
<pin name="PGND@6" direction="in"/>
</symbol>
<symbol name="TL7660">
<pin name="CAP+" direction="pas"/>
<pin name="CAP-" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="LV" direction="pas"/>
<pin name="VOUT" direction="pas"/>
<pin name="OSC" direction="in"/>
</symbol>
<symbol name="PCM1792">
<pin name="ZEROL"/>
<pin name="ZEROR"/>
<pin name="MSEL" direction="in"/>
<pin name="LRCK" direction="in"/>
<pin name="DATA" direction="in"/>
<pin name="BCK" direction="in"/>
<pin name="SCK" direction="in"/>
<pin name="DGND" direction="in"/>
<pin name="VDD" direction="in"/>
<pin name="!MS"/>
<pin name="MDI" direction="in"/>
<pin name="MC" direction="in"/>
<pin name="MDO"/>
<pin name="!RST" direction="in"/>
<pin name="VCC2R" direction="in"/>
<pin name="AGND3R" direction="in"/>
<pin name="IOUTR+" direction="out"/>
<pin name="IOUTR-" direction="out"/>
<pin name="AGND1" direction="in"/>
<pin name="IREF" direction="out"/>
<pin name="VCOMR" direction="in"/>
<pin name="VCOML" direction="in"/>
<pin name="VCC1" direction="in"/>
<pin name="AGND2" direction="in"/>
<pin name="IOUTL+" direction="out"/>
<pin name="IOUTL-" direction="out"/>
<pin name="AGND3L" direction="in"/>
<pin name="VCC2L" direction="in"/>
</symbol>
<symbol name="PCM4220">
<pin name="AGND" direction="pwr"/>
<pin name="VINR-" direction="in"/>
<pin name="VINR+" direction="in"/>
<pin name="VCC1" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VINL-" direction="in"/>
<pin name="VINL+" direction="in"/>
<pin name="AGND@5" direction="pwr"/>
<pin name="VCOML" direction="out"/>
<pin name="REFGNDL" direction="pwr"/>
<pin name="VREFL" direction="out"/>
<pin name="PCMEN" direction="in"/>
<pin name="HPFDR" direction="in"/>
<pin name="HPFDL" direction="in"/>
<pin name="FS0" direction="in"/>
<pin name="FS1" direction="in"/>
<pin name="DF" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="SUB1" direction="in"/>
<pin name="SUB0" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="DATA" direction="out"/>
<pin name="BCK"/>
<pin name="LRCK"/>
<pin name="MCKI" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="OVFL" direction="out"/>
<pin name="OVFR" direction="out"/>
<pin name="S/M" direction="in"/>
<pin name="DGND@4" direction="out"/>
<pin name="OWL1" direction="in"/>
<pin name="OWL0" direction="in"/>
<pin name="FMT1" direction="in"/>
<pin name="FMT0" direction="in"/>
<pin name="DGND@5" direction="pwr"/>
<pin name="VREFR" direction="out"/>
<pin name="REFGNDR" direction="pwr"/>
<pin name="VCOMR" direction="out"/>
</symbol>
<symbol name="PCM4222">
<pin name="AGND" direction="pwr"/>
<pin name="VIN-" direction="in"/>
<pin name="VINR+" direction="in"/>
<pin name="VCC1" direction="pwr"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="VINL-" direction="in"/>
<pin name="VINL+" direction="in"/>
<pin name="AGND@5" direction="pwr"/>
<pin name="VCOML" direction="out"/>
<pin name="REFGNDL" direction="pwr"/>
<pin name="VREFL" direction="out"/>
<pin name="PCMEN" direction="in"/>
<pin name="HPFDR/MOD1"/>
<pin name="HPFDL/MOD2"/>
<pin name="FS0/MOD3"/>
<pin name="FS1/MOD4"/>
<pin name="DF/MOD5"/>
<pin name="DSDEN/MOD6"/>
<pin name="MODEN" direction="in"/>
<pin name="DSDMODE" direction="in"/>
<pin name="SUB1/MCKO"/>
<pin name="SUB0/WCKO"/>
<pin name="DSDCLK" direction="out"/>
<pin name="DSDL" direction="out"/>
<pin name="DSDR" direction="out"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="DATA" direction="out"/>
<pin name="BCK"/>
<pin name="LRCK"/>
<pin name="MCKI" direction="in"/>
<pin name="RST" direction="in"/>
<pin name="OVFL" direction="out"/>
<pin name="OVFR" direction="out"/>
<pin name="S/M" direction="in"/>
<pin name="DGND@1" direction="out"/>
<pin name="OWL1" direction="in"/>
<pin name="OWL0" direction="in"/>
<pin name="FMT1" direction="in"/>
<pin name="FMT0" direction="in"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="VREFR" direction="out"/>
<pin name="REFGNDR" direction="pwr"/>
<pin name="VCOMR" direction="out"/>
</symbol>
<symbol name="PCM4204">
<pin name="VIN1-" direction="in"/>
<pin name="VIN1+" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="VCC1" direction="pwr"/>
<pin name="AGND1" direction="pwr"/>
<pin name="BGND1" direction="pwr"/>
<pin name="DGND1" direction="pwr"/>
<pin name="VDD1" direction="pwr"/>
<pin name="RST" direction="in"/>
<pin name="TEST" direction="in"/>
<pin name="FS0" direction="in"/>
<pin name="FS1" direction="in"/>
<pin name="FS2" direction="in"/>
<pin name="SCKI" direction="in"/>
<pin name="BGND2" direction="pwr"/>
<pin name="S/M" direction="in"/>
<pin name="FMT0" direction="in"/>
<pin name="FMT1" direction="in"/>
<pin name="FMT2" direction="in"/>
<pin name="NC@2" direction="nc"/>
<pin name="DGND2" direction="pwr"/>
<pin name="VDD2" direction="pwr"/>
<pin name="DSDCLK"/>
<pin name="DSD1"/>
<pin name="DSD2"/>
<pin name="DSD3"/>
<pin name="DSD4"/>
<pin name="BCK"/>
<pin name="LRCK"/>
<pin name="SDOUT1" direction="out"/>
<pin name="SDOUT2" direction="out"/>
<pin name="BGND3" direction="pwr"/>
<pin name="CLIP1" direction="out"/>
<pin name="CLIP2" direction="out"/>
<pin name="CLIP3" direction="out"/>
<pin name="CLIP4" direction="out"/>
<pin name="HPFD" direction="in"/>
<pin name="SUB" direction="in"/>
<pin name="VDD3" direction="pwr"/>
<pin name="DGND3" direction="pwr"/>
<pin name="BGND4" direction="pwr"/>
<pin name="AGND2" direction="pwr"/>
<pin name="VCC2" direction="pwr"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="VIN4-" direction="in"/>
<pin name="VIN4+" direction="in"/>
<pin name="VREF34+" direction="out"/>
<pin name="VREF34-" direction="out"/>
<pin name="AGND3" direction="out"/>
<pin name="VCOM34" direction="out"/>
<pin name="NC@5" direction="nc"/>
<pin name="VIN3-" direction="in"/>
<pin name="VIN3+" direction="in"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="VIN2-" direction="in"/>
<pin name="VIN2+" direction="in"/>
<pin name="NC@8" direction="nc"/>
<pin name="VCOM12" direction="out"/>
<pin name="AGND4" direction="pwr"/>
<pin name="VREF12-" direction="out"/>
<pin name="VREF12+" direction="out"/>
<pin name="EXP" direction="out"/>
</symbol>
<symbol name="PCM1804">
<pin name="VREFL" direction="pwr"/>
<pin name="AGNDL" direction="pwr"/>
<pin name="VCOML" direction="pwr"/>
<pin name="VINL+" direction="in"/>
<pin name="VINL-" direction="in"/>
<pin name="FMT0" direction="in"/>
<pin name="FMT1" direction="in"/>
<pin name="S/!M" direction="in"/>
<pin name="OSR0" direction="in"/>
<pin name="OSR1" direction="in"/>
<pin name="OSR2" direction="in"/>
<pin name="BYPAS" direction="in"/>
<pin name="DGND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="DATA/DSDR" direction="out"/>
<pin name="SCKI" direction="in"/>
<pin name="!RST" direction="in"/>
<pin name="OVFR" direction="out"/>
<pin name="OVFL" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="VINR-" direction="in"/>
<pin name="VINR+" direction="in"/>
<pin name="VCOMR" direction="pwr"/>
<pin name="AGNDR" direction="pwr"/>
<pin name="VREFR" direction="pwr"/>
<pin name="BCK/DSDL"/>
<pin name="LRCK/DSDBCK"/>
</symbol>
<symbol name="SN65LVDS125A">
<pin name="1A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="4B" direction="in"/>
<pin name="1DE" direction="in"/>
<pin name="2DE" direction="in"/>
<pin name="3DE" direction="in"/>
<pin name="4DE" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="1Z" direction="out" function="dot"/>
<pin name="2Z" direction="out" function="dot"/>
<pin name="3Z" direction="out" function="dot"/>
<pin name="4Z" direction="out" function="dot"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="4Y" direction="out"/>
<pin name="S10" direction="in"/>
<pin name="S11" direction="in"/>
<pin name="S20" direction="in"/>
<pin name="S21" direction="in"/>
<pin name="S30" direction="in"/>
<pin name="S31" direction="in"/>
<pin name="S40" direction="in"/>
<pin name="S41" direction="in"/>
</symbol>
<symbol name="VCC4-GND6">
<pin name="VCC@1" direction="in"/>
<pin name="VCC@2" direction="in"/>
<pin name="VCC@3" direction="in"/>
<pin name="VCC@4" direction="in"/>
<pin name="GND@1" direction="in"/>
<pin name="GND@2" direction="in"/>
<pin name="GND@3" direction="in"/>
<pin name="GND@4" direction="in"/>
<pin name="GND@5" direction="in"/>
<pin name="GND@6" direction="in"/>
</symbol>
<symbol name="ADS1274">
<pin name="AINP2" direction="in"/>
<pin name="AINN2" direction="in"/>
<pin name="AINP1" direction="in"/>
<pin name="AINN1" direction="in"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AGND" direction="pwr"/>
<pin name="DGND" direction="pwr"/>
<pin name="TEST0" direction="in"/>
<pin name="TEST1" direction="in"/>
<pin name="CLKDIV" direction="in"/>
<pin name="!SYNC" direction="in"/>
<pin name="DIN" direction="in"/>
<pin name="DOUT8" direction="out"/>
<pin name="DOUT7" direction="out"/>
<pin name="DOUT6" direction="out"/>
<pin name="DOUT5" direction="out"/>
<pin name="DOUT4" direction="out"/>
<pin name="DOUT3" direction="out"/>
<pin name="DOUT2" direction="out"/>
<pin name="DOUT1" direction="out"/>
<pin name="DGND@1" direction="pwr"/>
<pin name="IOVDD" direction="pwr"/>
<pin name="IOVDD@1" direction="pwr"/>
<pin name="DGND@2" direction="pwr"/>
<pin name="DGND@3" direction="pwr"/>
<pin name="DVDD" direction="pwr"/>
<pin name="CLK" direction="in"/>
<pin name="SCLK"/>
<pin name="!DRDY!/FSYNC"/>
<pin name="FORMAT2" direction="in"/>
<pin name="FORMAT1" direction="in"/>
<pin name="FORMAT0" direction="in"/>
<pin name="MODE1" direction="in"/>
<pin name="MODE0" direction="in"/>
<pin name="!PWDN8" direction="in"/>
<pin name="!PWDN7" direction="in"/>
<pin name="!PWDN6" direction="in"/>
<pin name="!PWDN5" direction="in"/>
<pin name="!PWDN4" direction="in"/>
<pin name="!PWDN3" direction="in"/>
<pin name="!PWDN2" direction="in"/>
<pin name="!PWDN1" direction="in"/>
<pin name="AGND@1" direction="pwr"/>
<pin name="AVDD@1" direction="pwr"/>
<pin name="EDS@8" direction="in"/>
<pin name="EDS@4" direction="in"/>
<pin name="EDS@7" direction="in"/>
<pin name="EDS@3" direction="in"/>
<pin name="EDS@6" direction="in"/>
<pin name="EDS@2" direction="in"/>
<pin name="EDS@5" direction="in"/>
<pin name="EDS@1" direction="in"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="AGND@2" direction="pwr"/>
<pin name="VCOM" direction="out"/>
<pin name="VREFP" direction="in"/>
<pin name="VREFN" direction="in"/>
<pin name="AGND@3" direction="pwr"/>
<pin name="AGND@4" direction="pwr"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="AINP4" direction="in"/>
<pin name="AINN4" direction="in"/>
<pin name="AINP3" direction="in"/>
<pin name="AINN3" direction="in"/>
</symbol>
<symbol name="EXP25">
<pin name="EXP@1" direction="pas"/>
<pin name="EXP@2" direction="pas"/>
<pin name="EXP@3" direction="pas"/>
<pin name="EXP@4" direction="pas"/>
<pin name="EXP@5" direction="pas"/>
<pin name="EXP@6" direction="pas"/>
<pin name="EXP@7" direction="pas"/>
<pin name="EXP@8" direction="pas"/>
<pin name="EXP@9" direction="pas"/>
<pin name="EXP@10" direction="pas"/>
<pin name="EXP@11" direction="pas"/>
<pin name="EXP@12" direction="pas"/>
<pin name="EXP@13" direction="pas"/>
<pin name="EXP@14" direction="pas"/>
<pin name="EXP@15" direction="pas"/>
<pin name="EXP@16" direction="pas"/>
<pin name="EXP@17" direction="pas"/>
<pin name="EXP@18" direction="pas"/>
<pin name="EXP@19" direction="pas"/>
<pin name="EXP@20" direction="pas"/>
<pin name="EXP@21" direction="pas"/>
<pin name="EXP@22" direction="pas"/>
<pin name="EXP@23" direction="pas"/>
<pin name="EXP@24" direction="pas"/>
<pin name="EXP@25" direction="pas"/>
</symbol>
<symbol name="OMAP-L138_ZCE">
<pin name="NMIN" direction="in"/>
<pin name="LCDACENBCSN_GP60"/>
<pin name="VPIFCLKO3_GP61"/>
<pin name="VPIFCLKIN3_MMCSD1DAT1_GP62"/>
<pin name="VPIFCLKO2_MMCSD1DAT2_GP63"/>
<pin name="VPIFCLKIN2_MMCSD1DAT3_GP64"/>
<pin name="MMCSD1DAT4_LCDVSYNC_GP88"/>
<pin name="MMCSD1DAT5_LCDHSYNC_GP89"/>
<pin name="MMCSD1DAT6_LCDMCLK_GP810"/>
<pin name="MMCSD1DAT7_LCDPCLK_GP811"/>
<pin name="UPPCHBWAIT_GP812"/>
<pin name="MMCSD1CMD_UPPCHBENABLE_GP813"/>
<pin name="MMCSD1CLK_UPPCHBSTART_GP814"/>
<pin name="MMCSD1DAT0_UPPCHBCLOCK_GP815"/>
<pin name="VPIFDOUT8_LCDD8_UPPXD0_GP70_BOOT0"/>
<pin name="VPIFDOUT9_LCDD9_UPPXD1_GP71_BOOT1"/>
<pin name="VPIFDOUT10_LCDD10_UPPXD2_GP72_BOOT2"/>
<pin name="VPIFDOUT11_LCDD11_UPPXD3_GP73_BOOT3"/>
<pin name="VPIFDOUT12_LCDD12_UPPXD4_GP74_BOOT4"/>
<pin name="VPIFDOUT13_LCDD13_UPPXD5_GP75_BOOT5"/>
<pin name="VPIFDOUT14_LCDD14_UPPXD6_GP76_BOOT6"/>
<pin name="VPIFDOUT15_LCDD15_UPPXD7_GP77_BOOT7"/>
<pin name="VPIFDOUT0_LCDD0_UPPXD8_GP78"/>
<pin name="VPIFDOUT1_LCDD1_UPPXD9_GP79"/>
<pin name="VPIFDOUT2_LCDD2_UPPXD10_GP710"/>
<pin name="VPIFDOUT3_LCDD3_UPPXD11_GP711"/>
<pin name="VPIFDOUT4_LCDD4_UPPXD12_GP712"/>
<pin name="VPIFDOUT5_LCDD5_UPPXD13_GP713"/>
<pin name="VPIFDOUT6_LCDD6_UPPXD14_GP714"/>
<pin name="VPIFDOUT7_LCDD7_UPPXD15_GP715"/>
<pin name="VPIFDIN8_UHPIHD0_UPPD0_GP65"/>
<pin name="VPIFDIN9_UHPIHD1_UPPD1"/>
<pin name="VPIFDIN10_UHPIHD2_UPPD2"/>
<pin name="VPIFDIN11_UHPIHD3_UPPD3"/>
<pin name="VPIFDIN12_UHPIHD4_UPPD4"/>
<pin name="VPIFDIN13FIELD_UHPIHD5_UPPD5"/>
<pin name="VPIFDIN14HSYNC_UHPIHD6_UPPD6"/>
<pin name="VPIFDIN15VSYNC_UHPIHD7_UPPD7"/>
<pin name="VPIFDIN0_UHPIHD8_UPPD8_RMIICRSDV"/>
<pin name="VPIFDIN1_UHPIHD9_UPPD9_RMIIMHZ50CLK"/>
<pin name="VPIFDIN2_UHPIHD10_UPPD10_RMIIRXER"/>
<pin name="VPIFDIN3_UHPIHD11_UPPD11_RMIIRXD0"/>
<pin name="VPIFDIN4_UHPIHD12_UPPD12_RMIIRXD1"/>
<pin name="VPIFDIN5_UHPIHD13_UPPD13_RMIITXEN"/>
<pin name="VPIFDIN6_UHPIHD14_UPPD14_RMIITXD0"/>
<pin name="VPIFDIN7_UHPIHD15_UPPD15_RMIITXD1"/>
<pin name="VPIFCLKIN1_UHPIHDS1N_GP66"/>
<pin name="VPIFCLKIN0_UHPIHCSN_GP67_UPP2XTXCLK"/>
<pin name="UHPIHRWN_UPPCHAWAIT_GP68"/>
<pin name="UHPIHHWIL_UPPCHAENABLE_GP69"/>
<pin name="UHPIHCNTL1_UPPCHASTART_GP610"/>
<pin name="UHPIHCNTL0_UPPCHACLOCK_GP611"/>
<pin name="UHPIHINTN_GP612"/>
<pin name="UHPIHRDYN_GP613"/>
<pin name="CLKOUT_UHPIHDS2N_GP614"/>
<pin name="RESETOUTN_UHPIHASN_GP615"/>
<pin name="EMAA0_GP50"/>
<pin name="EMAA1_GP51"/>
<pin name="EMAA2_GP52"/>
<pin name="EMAA3_GP53"/>
<pin name="EMAA4_GP54"/>
<pin name="EMAA5_GP55"/>
<pin name="EMAA6_GP56"/>
<pin name="EMAA7_GP57"/>
<pin name="EMAA8_GP58"/>
<pin name="EMAA9_GP59"/>
<pin name="EMAA10_GP510"/>
<pin name="EMAA11_GP511"/>
<pin name="EMAA12_GP512"/>
<pin name="EMAA13_GP513"/>
<pin name="EMAA14_MMCSD0DAT7_GP514"/>
<pin name="EMAA15_MMCSD0DAT6_GP515"/>
<pin name="EMAA16_MMCSD0DAT5_GP40"/>
<pin name="EMAA17_MMCSD0DAT4_GP41"/>
<pin name="EMAA18_MMCSD0DAT3_GP42"/>
<pin name="EMAA19_MMCSD0DAT2_GP43"/>
<pin name="EMAA20_MMCSD0DAT1_GP44"/>
<pin name="EMAA21_MMCSD0DAT0_GP45"/>
<pin name="EMAA22_MMCSD0CMD_GP46"/>
<pin name="EMAA23_MMCSD0CLK_GP47"/>
<pin name="EMAD0_GP48"/>
<pin name="EMAD1_GP49"/>
<pin name="EMAD2_GP410"/>
<pin name="EMAD3_GP411"/>
<pin name="EMAD4_GP412"/>
<pin name="EMAD5_GP413"/>
<pin name="EMAD6_GP414"/>
<pin name="EMAD7_GP415"/>
<pin name="EMAD8_GP30"/>
<pin name="EMAD9_GP31"/>
<pin name="EMAD10_GP32"/>
<pin name="EMAD11_GP33"/>
<pin name="EMAD12_GP34"/>
<pin name="EMAD13_GP35"/>
<pin name="EMAD14_GP36"/>
<pin name="EMAD15_GP37"/>
<pin name="EMAWAIT0_GP38"/>
<pin name="EMARNW_GP39"/>
<pin name="EMAOEN_GP310"/>
<pin name="EMAWEN_GP311"/>
<pin name="EMACS5N_GP212"/>
<pin name="EMACS4N_GP313"/>
<pin name="EMACS3N_GP314"/>
<pin name="EMACS2N_GP315"/>
<pin name="EMACS0N_GP20"/>
<pin name="EMAWAIT1_GP21"/>
<pin name="EMAWEDQM1N_GP22"/>
<pin name="EMAWEDQM0N_GP23"/>
<pin name="EMACASN_GP24"/>
<pin name="EMARASN_GP25"/>
<pin name="EMASDCKE_GP26"/>
<pin name="EMACLK_GP27"/>
<pin name="EMABA0_GP28"/>
<pin name="EMABA1_GP29"/>
<pin name="SPI1SIMO_GP210"/>
<pin name="SPI1SOMI_GP211"/>
<pin name="SPI1ENAN_GP212"/>
<pin name="SPI1CLK_GP213"/>
<pin name="SPI1SCS0N_EPWM1B_GP214_TM64P3IN12"/>
<pin name="SPI1SCS1N_EPWM1A_GP215_TM64P2IN12"/>
<pin name="SPI1SCS2N_UART1TXD_SATACPPOD_GP10"/>
<pin name="SPI1SCS3N_UART1RXD_SATALED_GP11"/>
<pin name="SPI1SCS4N_UART2TXD_I2C1SDA_GP12"/>
<pin name="SPI1SCS5N_UART2RXD_I2C1SCL_GP13"/>
<pin name="SPI1SCS6N_I2C0SDA_TM64P3OUT12_GP14"/>
<pin name="SPI1SCS7N_I2C0SCL_TM64P2OUT12_GP15"/>
<pin name="SPI0SCS0N_TM64P1OUT12_GP16_MDIOD_TM64P1IN12"/>
<pin name="SPI0SCS1N_TM64P0OUT12_GP17_MDIOCLK_TM64P0IN12"/>
<pin name="SPI0SCS2N_UART0RTS_GP81_MIIRXD0_SATACPDET"/>
<pin name="SPI0SCS3N_UART0CTS_GP82_MIIRXD1_SATAMPSWITCH"/>
<pin name="SPI0SCS4N_UART0TXD_GP83_MIIRXD2"/>
<pin name="SPI0SCS5N_UART0RXD_GP84_MIIRXD3"/>
<pin name="SPI0SIMO_EPWMSYNC0_GP85_MIICRS"/>
<pin name="SPI0SOMI_EPWMSYNCI_GP86_MIIRXER"/>
<pin name="SPI0ENAN_EPWM0B_MIIRXDV"/>
<pin name="SPI0CLK_EPWM0A_GP18_MIIRXCLK"/>
<pin name="AXR00_ECAP0APWM0_GP87_MIITXD0_CLKS0"/>
<pin name="AXR01_DX0_GP19MIITXD1"/>
<pin name="AXR02_DR0_GP110_MIITXD2"/>
<pin name="AXR03_FSX0_GP111_MIITXD3"/>
<pin name="AXR04_FSR0_GP112_MIICOL"/>
<pin name="AXR05_CLKX0_GP113_MIITXCLK"/>
<pin name="AXR06_CLKR0_GP114_MIITXEN"/>
<pin name="AXR07_EPWM1TZ0_GP115"/>
<pin name="AXR08_CLKS1_ECAP1APWM1_GP00"/>
<pin name="AXR09_DX1_GP01"/>
<pin name="AXR010_DR1_GP02"/>
<pin name="AXR011_FSX1_GP03"/>
<pin name="AXR012_FSR1_GP04"/>
<pin name="AXR013_CLKX1_GP05"/>
<pin name="AXR014_CLKR1_GP06"/>
<pin name="AXR015_EPWM0TZ0_ECAP2APWM2_GP07"/>
<pin name="AMUTEIN_RTCALARM_UART2CTS_GP08_DEEPSLEEPN"/>
<pin name="AMUTE_UART2RTS_GP09"/>
<pin name="AHCLKX_USBREFCLKIN_UART1CTS_GP010"/>
<pin name="AHCLKR_UART1RTS_GP011"/>
<pin name="AFSX0_GP012"/>
<pin name="AFSR0_GP013"/>
<pin name="ACLKX_GP014"/>
<pin name="ACLKR_GP015"/>
<pin name="USB0DRVVBUS"/>
<pin name="EMU1"/>
<pin name="EMU0"/>
<pin name="DDRDQGATE1"/>
<pin name="DDRDQGATE0"/>
<pin name="DDRDQS0"/>
<pin name="DDRDQS1"/>
<pin name="DDRDQM0N"/>
<pin name="DDRDQM1N"/>
<pin name="DDRD15"/>
<pin name="DDRD14"/>
<pin name="DDRD13"/>
<pin name="DDRD12"/>
<pin name="DDRD11"/>
<pin name="DDRD10"/>
<pin name="DDRD9"/>
<pin name="DDRD8"/>
<pin name="DDRD7"/>
<pin name="DDRD6"/>
<pin name="DDRD5"/>
<pin name="DDRD4"/>
<pin name="DDRD3"/>
<pin name="DDRD2"/>
<pin name="DDRD1"/>
<pin name="DDRD0"/>
<pin name="DDRA13"/>
<pin name="DDRA12"/>
<pin name="DDRA11"/>
<pin name="DDRA10"/>
<pin name="DDRA9"/>
<pin name="DDRA8"/>
<pin name="DDRA7"/>
<pin name="DDRA6"/>
<pin name="DDRA5"/>
<pin name="DDRA4"/>
<pin name="DDRA3"/>
<pin name="DDRA2"/>
<pin name="DDRA1"/>
<pin name="DDRA0"/>
<pin name="DDRBA0"/>
<pin name="DDRBA1"/>
<pin name="DDRBA2"/>
<pin name="DDRWEN"/>
<pin name="DDRRASN"/>
<pin name="DDRCASN"/>
<pin name="DDRCSN"/>
<pin name="DDRCLKN"/>
<pin name="DDRCLKP"/>
<pin name="DDRCKE"/>
<pin name="SATARXN" direction="in"/>
<pin name="SATARXP" direction="in"/>
<pin name="SATATXP" direction="hiz"/>
<pin name="RESETN" direction="in"/>
<pin name="TRSTN" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="VDD@31" direction="pwr"/>
<pin name="VDD@32" direction="pwr"/>
<pin name="VDD@33" direction="pwr"/>
<pin name="VDD@34" direction="pwr"/>
<pin name="VDD@35" direction="pwr"/>
<pin name="VDD@36" direction="pwr"/>
<pin name="VDD@37" direction="pwr"/>
<pin name="VDD@38" direction="pwr"/>
<pin name="VDD@39" direction="pwr"/>
<pin name="VDD@40" direction="pwr"/>
<pin name="VDD@41" direction="pwr"/>
<pin name="VDD@42" direction="pwr"/>
<pin name="VDD@43" direction="pwr"/>
<pin name="VDD@44" direction="pwr"/>
<pin name="VDD@45" direction="pwr"/>
<pin name="VDD@46" direction="pwr"/>
<pin name="VDD@47" direction="pwr"/>
<pin name="VDD@48" direction="pwr"/>
<pin name="VDD@49" direction="pwr"/>
<pin name="VDD@50" direction="pwr"/>
<pin name="VDD@51" direction="pwr"/>
<pin name="VDD@52" direction="pwr"/>
<pin name="VDD@53" direction="pwr"/>
<pin name="VDD@54" direction="pwr"/>
<pin name="VDD@55" direction="pwr"/>
<pin name="VDD@56" direction="pwr"/>
<pin name="VDD@57" direction="pwr"/>
<pin name="VDD@58" direction="pwr"/>
<pin name="VDD@59" direction="pwr"/>
<pin name="VDD@60" direction="pwr"/>
<pin name="VDD@61" direction="pwr"/>
<pin name="VDD@62" direction="pwr"/>
<pin name="VDD@63" direction="pwr"/>
<pin name="VDD@64" direction="pwr"/>
<pin name="VDD@65" direction="pwr"/>
<pin name="VDD@66" direction="pwr"/>
<pin name="VDD@67" direction="pwr"/>
<pin name="VDD@68" direction="pwr"/>
<pin name="VDD@69" direction="pwr"/>
<pin name="VDD@70" direction="pwr"/>
<pin name="VDD@71" direction="pwr"/>
<pin name="VDD@72" direction="pwr"/>
<pin name="VDD@73" direction="pwr"/>
<pin name="VDD@74" direction="pwr"/>
<pin name="VDD@75" direction="pwr"/>
<pin name="VDD@76" direction="pwr"/>
<pin name="VDD@77" direction="pwr"/>
<pin name="VDD@78" direction="pwr"/>
<pin name="VDD@79" direction="pwr"/>
<pin name="VDD@80" direction="pwr"/>
<pin name="VDD@81" direction="pwr"/>
<pin name="VDD@82" direction="pwr"/>
<pin name="VDD@83" direction="pwr"/>
<pin name="VDD@84" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
</symbol>
<symbol name="OMAPL138ZWT">
<pin name="NMIN" direction="in"/>
<pin name="LCDACENBCSN_GP60"/>
<pin name="VPIFCLKO3_GP61"/>
<pin name="VPIFCLKIN3_MMCSD1DAT1_GP62"/>
<pin name="VPIFCLKO2_MMCSD1DAT2_GP63"/>
<pin name="VPIFCLKIN2_MMCSD1DAT3_GP64"/>
<pin name="MMCSD1DAT4_LCDVSYNC_GP88"/>
<pin name="MMCSD1DAT5_LCDHSYNC_GP89"/>
<pin name="MMCSD1DAT6_LCDMCLK_GP810"/>
<pin name="MMCSD1DAT7_LCDPCLK_GP811"/>
<pin name="UPPCHBWAIT_GP812"/>
<pin name="MMCSD1CMD_UPPCHBENABLE_GP813"/>
<pin name="MMCSD1CLK_UPPCHBSTART_GP814"/>
<pin name="MMCSD1DAT0_UPPCHBCLOCK_GP815"/>
<pin name="VPIFDOUT8_LCDD8_UPPXD0_GP70_BOOT0"/>
<pin name="VPIFDOUT9_LCDD9_UPPXD1_GP71_BOOT1"/>
<pin name="VPIFDOUT10_LCDD10_UPPXD2_GP72_BOOT2"/>
<pin name="VPIFDOUT11_LCDD11_UPPXD3_GP73_BOOT3"/>
<pin name="VPIFDOUT12_LCDD12_UPPXD4_GP74_BOOT4"/>
<pin name="VPIFDOUT13_LCDD13_UPPXD5_GP75_BOOT5"/>
<pin name="VPIFDOUT14_LCDD14_UPPXD6_GP76_BOOT6"/>
<pin name="VPIFDOUT15_LCDD15_UPPXD7_GP77_BOOT7"/>
<pin name="VPIFDOUT0_LCDD0_UPPXD8_GP78"/>
<pin name="VPIFDOUT1_LCDD1_UPPXD9_GP79"/>
<pin name="VPIFDOUT2_LCDD2_UPPXD10_GP710"/>
<pin name="VPIFDOUT3_LCDD3_UPPXD11_GP711"/>
<pin name="VPIFDOUT4_LCDD4_UPPXD12_GP712"/>
<pin name="VPIFDOUT5_LCDD5_UPPXD13_GP713"/>
<pin name="VPIFDOUT6_LCDD6_UPPXD14_GP714"/>
<pin name="VPIFDOUT7_LCDD7_UPPXD15_GP715"/>
<pin name="VPIFDIN8_UHPIHD0_UPPD0_GP65"/>
<pin name="VPIFDIN9_UHPIHD1_UPPD1"/>
<pin name="VPIFDIN10_UHPIHD2_UPPD2"/>
<pin name="VPIFDIN11_UHPIHD3_UPPD3"/>
<pin name="VPIFDIN12_UHPIHD4_UPPD4"/>
<pin name="VPIFDIN13FIELD_UHPIHD5_UPPD5"/>
<pin name="VPIFDIN14HSYNC_UHPIHD6_UPPD6"/>
<pin name="VPIFDIN15VSYNC_UHPIHD7_UPPD7"/>
<pin name="VPIFDIN0_UHPIHD8_UPPD8_RMIICRSDV"/>
<pin name="VPIFDIN1_UHPIHD9_UPPD9_RMIIMHZ50CLK"/>
<pin name="VPIFDIN2_UHPIHD10_UPPD10_RMIIRXER"/>
<pin name="VPIFDIN3_UHPIHD11_UPPD11_RMIIRXD0"/>
<pin name="VPIFDIN4_UHPIHD12_UPPD12_RMIIRXD1"/>
<pin name="VPIFDIN5_UHPIHD13_UPPD13_RMIITXEN"/>
<pin name="VPIFDIN6_UHPIHD14_UPPD14_RMIITXD0"/>
<pin name="VPIFDIN7_UHPIHD15_UPPD15_RMIITXD1"/>
<pin name="VPIFCLKIN1_UHPIHDS1N_GP66"/>
<pin name="VPIFCLKIN0_UHPIHCSN_GP67_UPP2XTXCLK"/>
<pin name="UHPIHRWN_UPPCHAWAIT_GP68"/>
<pin name="UHPIHHWIL_UPPCHAENABLE_GP69"/>
<pin name="UHPIHCNTL1_UPPCHASTART_GP610"/>
<pin name="UHPIHCNTL0_UPPCHACLOCK_GP611"/>
<pin name="UHPIHINTN_GP612"/>
<pin name="UHPIHRDYN_GP613"/>
<pin name="CLKOUT_UHPIHDS2N_GP614"/>
<pin name="RESETOUTN_UHPIHASN_GP615"/>
<pin name="EMAA0_GP50"/>
<pin name="EMAA1_GP51"/>
<pin name="EMAA2_GP52"/>
<pin name="EMAA3_GP53"/>
<pin name="EMAA4_GP54"/>
<pin name="EMAA5_GP55"/>
<pin name="EMAA6_GP56"/>
<pin name="EMAA7_GP57"/>
<pin name="EMAA8_GP58"/>
<pin name="EMAA9_GP59"/>
<pin name="EMAA10_GP510"/>
<pin name="EMAA11_GP511"/>
<pin name="EMAA12_GP512"/>
<pin name="EMAA13_GP513"/>
<pin name="EMAA14_MMCSD0DAT7_GP514"/>
<pin name="EMAA15_MMCSD0DAT6_GP515"/>
<pin name="EMAA16_MMCSD0DAT5_GP40"/>
<pin name="EMAA17_MMCSD0DAT4_GP41"/>
<pin name="EMAA18_MMCSD0DAT3_GP42"/>
<pin name="EMAA19_MMCSD0DAT2_GP43"/>
<pin name="EMAA20_MMCSD0DAT1_GP44"/>
<pin name="EMAA21_MMCSD0DAT0_GP45"/>
<pin name="EMAA22_MMCSD0CMD_GP46"/>
<pin name="EMAA23_MMCSD0CLK_GP47"/>
<pin name="EMAD0_GP48"/>
<pin name="EMAD1_GP49"/>
<pin name="EMAD2_GP410"/>
<pin name="EMAD3_GP411"/>
<pin name="EMAD4_GP412"/>
<pin name="EMAD5_GP413"/>
<pin name="EMAD6_GP414"/>
<pin name="EMAD7_GP415"/>
<pin name="EMAD8_GP30"/>
<pin name="EMAD9_GP31"/>
<pin name="EMAD10_GP32"/>
<pin name="EMAD11_GP33"/>
<pin name="EMAD12_GP34"/>
<pin name="EMAD13_GP35"/>
<pin name="EMAD14_GP36"/>
<pin name="EMAD15_GP37"/>
<pin name="EMAWAIT0_GP38"/>
<pin name="EMARNW_GP39"/>
<pin name="EMAOEN_GP310"/>
<pin name="EMAWEN_GP311"/>
<pin name="EMACS5N_GP212"/>
<pin name="EMACS4N_GP313"/>
<pin name="EMACS3N_GP314"/>
<pin name="EMACS2N_GP315"/>
<pin name="EMACS0N_GP20"/>
<pin name="EMAWAIT1_GP21"/>
<pin name="EMAWEDQM1N_GP22"/>
<pin name="EMAWEDQM0N_GP23"/>
<pin name="EMACASN_GP24"/>
<pin name="EMARASN_GP25"/>
<pin name="EMASDCKE_GP26"/>
<pin name="EMACLK_GP27"/>
<pin name="EMABA0_GP28"/>
<pin name="EMABA1_GP29"/>
<pin name="SPI1SIMO_GP210"/>
<pin name="SPI1SOMI_GP211"/>
<pin name="SPI1ENAN_GP212"/>
<pin name="SPI1CLK_GP213"/>
<pin name="SPI1SCS0N_EPWM1B_GP214_TM64P3IN12"/>
<pin name="SPI1SCS1N_EPWM1A_GP215_TM64P2IN12"/>
<pin name="SPI1SCS2N_UART1TXD_SATACPPOD_GP10"/>
<pin name="SPI1SCS3N_UART1RXD_SATALED_GP11"/>
<pin name="SPI1SCS4N_UART2TXD_I2C1SDA_GP12"/>
<pin name="SPI1SCS5N_UART2RXD_I2C1SCL_GP13"/>
<pin name="SPI1SCS6N_I2C0SDA_TM64P3OUT12_GP14"/>
<pin name="SPI1SCS7N_I2C0SCL_TM64P2OUT12_GP15"/>
<pin name="SPI0SCS0N_TM64P1OUT12_GP16_MDIOD_TM64P1IN12"/>
<pin name="SPI0SCS1N_TM64P0OUT12_GP17_MDIOCLK_TM64P0IN12"/>
<pin name="SPI0SCS2N_UART0RTS_GP81_MIIRXD0_SATACPDET"/>
<pin name="SPI0SCS3N_UART0CTS_GP82_MIIRXD1_SATAMPSWITCH"/>
<pin name="SPI0SCS4N_UART0TXD_GP83_MIIRXD2"/>
<pin name="SPI0SCS5N_UART0RXD_GP84_MIIRXD3"/>
<pin name="SPI0SIMO_EPWMSYNC0_GP85_MIICRS"/>
<pin name="SPI0SOMI_EPWMSYNCI_GP86_MIIRXER"/>
<pin name="SPI0ENAN_EPWM0B_MIIRXDV"/>
<pin name="SPI0CLK_EPWM0A_GP18_MIIRXCLK"/>
<pin name="AXR00_ECAP0APWM0_GP87_MIITXD0_CLKS0"/>
<pin name="AXR01_DX0_GP19MIITXD1"/>
<pin name="AXR02_DR0_GP110_MIITXD2"/>
<pin name="AXR03_FSX0_GP111_MIITXD3"/>
<pin name="AXR04_FSR0_GP112_MIICOL"/>
<pin name="AXR05_CLKX0_GP113_MIITXCLK"/>
<pin name="AXR06_CLKR0_GP114_MIITXEN"/>
<pin name="AXR07_EPWM1TZ0_GP115"/>
<pin name="AXR08_CLKS1_ECAP1APWM1_GP00"/>
<pin name="AXR09_DX1_GP01"/>
<pin name="AXR010_DR1_GP02"/>
<pin name="AXR011_FSX1_GP03"/>
<pin name="AXR012_FSR1_GP04"/>
<pin name="AXR013_CLKX1_GP05"/>
<pin name="AXR014_CLKR1_GP06"/>
<pin name="AXR015_EPWM0TZ0_ECAP2APWM2_GP07"/>
<pin name="AMUTEIN_RTCALARM_UART2CTS_GP08_DEEPSLEEPN"/>
<pin name="AMUTE_UART2RTS_GP09"/>
<pin name="AHCLKX_USBREFCLKIN_UART1CTS_GP010"/>
<pin name="AHCLKR_UART1RTS_GP011"/>
<pin name="AFSX0_GP012"/>
<pin name="AFSR0_GP013"/>
<pin name="ACLKX_GP014"/>
<pin name="ACLKR_GP015"/>
<pin name="USB0DRVVBUS"/>
<pin name="EMU1"/>
<pin name="EMU0"/>
<pin name="DDRDQGATE1"/>
<pin name="DDRDQGATE0"/>
<pin name="DDRDQS0"/>
<pin name="DDRDQS1"/>
<pin name="DDRDQM0N"/>
<pin name="DDRDQM1N"/>
<pin name="DDRD15"/>
<pin name="DDRD14"/>
<pin name="DDRD13"/>
<pin name="DDRD12"/>
<pin name="DDRD11"/>
<pin name="DDRD10"/>
<pin name="DDRD9"/>
<pin name="DDRD8"/>
<pin name="DDRD7"/>
<pin name="DDRD6"/>
<pin name="DDRD5"/>
<pin name="DDRD4"/>
<pin name="DDRD3"/>
<pin name="DDRD2"/>
<pin name="DDRD1"/>
<pin name="DDRD0"/>
<pin name="DDRA13"/>
<pin name="DDRA12"/>
<pin name="DDRA11"/>
<pin name="DDRA10"/>
<pin name="DDRA9"/>
<pin name="DDRA8"/>
<pin name="DDRA7"/>
<pin name="DDRA6"/>
<pin name="DDRA5"/>
<pin name="DDRA4"/>
<pin name="DDRA3"/>
<pin name="DDRA2"/>
<pin name="DDRA1"/>
<pin name="DDRA0"/>
<pin name="DDRBA0"/>
<pin name="DDRBA1"/>
<pin name="DDRBA2"/>
<pin name="DDRWEN"/>
<pin name="DDRRASN"/>
<pin name="DDRCASN"/>
<pin name="DDRCSN"/>
<pin name="DDRCLKN"/>
<pin name="DDRCLKP"/>
<pin name="DDRCKE"/>
<pin name="SATARXN" direction="in"/>
<pin name="SATARXP" direction="in"/>
<pin name="SATATXP" direction="hiz"/>
<pin name="RESETN" direction="in"/>
<pin name="TRSTN" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="VDD@31" direction="pwr"/>
<pin name="VDD@32" direction="pwr"/>
<pin name="VDD@33" direction="pwr"/>
<pin name="VDD@34" direction="pwr"/>
<pin name="VDD@35" direction="pwr"/>
<pin name="VDD@36" direction="pwr"/>
<pin name="VDD@37" direction="pwr"/>
<pin name="VDD@38" direction="pwr"/>
<pin name="VDD@39" direction="pwr"/>
<pin name="VDD@40" direction="pwr"/>
<pin name="VDD@41" direction="pwr"/>
<pin name="VDD@42" direction="pwr"/>
<pin name="VDD@43" direction="pwr"/>
<pin name="VDD@44" direction="pwr"/>
<pin name="VDD@45" direction="pwr"/>
<pin name="VDD@46" direction="pwr"/>
<pin name="VDD@47" direction="pwr"/>
<pin name="VDD@48" direction="pwr"/>
<pin name="VDD@49" direction="pwr"/>
<pin name="VDD@50" direction="pwr"/>
<pin name="VDD@51" direction="pwr"/>
<pin name="VDD@52" direction="pwr"/>
<pin name="VDD@53" direction="pwr"/>
<pin name="VDD@54" direction="pwr"/>
<pin name="VDD@55" direction="pwr"/>
<pin name="VDD@56" direction="pwr"/>
<pin name="VDD@57" direction="pwr"/>
<pin name="VDD@58" direction="pwr"/>
<pin name="VDD@59" direction="pwr"/>
<pin name="VDD@60" direction="pwr"/>
<pin name="VDD@61" direction="pwr"/>
<pin name="VDD@62" direction="pwr"/>
<pin name="VDD@63" direction="pwr"/>
<pin name="VDD@64" direction="pwr"/>
<pin name="VDD@65" direction="pwr"/>
<pin name="VDD@66" direction="pwr"/>
<pin name="VDD@67" direction="pwr"/>
<pin name="VDD@68" direction="pwr"/>
<pin name="VDD@69" direction="pwr"/>
<pin name="VDD@70" direction="pwr"/>
<pin name="VDD@71" direction="pwr"/>
<pin name="VDD@72" direction="pwr"/>
<pin name="VDD@73" direction="pwr"/>
<pin name="VDD@74" direction="pwr"/>
<pin name="VDD@75" direction="pwr"/>
<pin name="VDD@76" direction="pwr"/>
<pin name="VDD@77" direction="pwr"/>
<pin name="VDD@78" direction="pwr"/>
<pin name="VDD@79" direction="pwr"/>
<pin name="VDD@80" direction="pwr"/>
<pin name="VDD@81" direction="pwr"/>
<pin name="VDD@82" direction="pwr"/>
<pin name="VDD@83" direction="pwr"/>
<pin name="VDD@84" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
</symbol>
<symbol name="OMAPL138Z-A">
<pin name="ACLKR_GP015"/>
<pin name="ACLKX_GP014"/>
<pin name="AFSR0_GP013"/>
<pin name="AFSX0_GP012"/>
<pin name="AHCLKR_UART1RTS_GP011"/>
<pin name="AHCLKX_USBREFCLKIN_UART1CTS_GP010"/>
<pin name="AMUTEIN_RTCALARM_UART2CTS_GP08_DEEPSLEEPN"/>
<pin name="AMUTE_UART2RTS_GP09"/>
<pin name="AXR00_ECAP0APWM0_GP87_MIITXD0_CLKS0"/>
<pin name="AXR01_DX0_GP19MIITXD1"/>
<pin name="AXR02_DR0_GP110_MIITXD2"/>
<pin name="AXR03_FSX0_GP111_MIITXD3"/>
<pin name="AXR04_FSR0_GP112_MIICOL"/>
<pin name="AXR05_CLKX0_GP113_MIITXCLK"/>
<pin name="AXR06_CLKR0_GP114_MIITXEN"/>
<pin name="AXR07_EPWM1TZ0_GP115"/>
<pin name="AXR08_CLKS1_ECAP1APWM1_GP00"/>
<pin name="AXR09_DX1_GP01"/>
<pin name="AXR010_DR1_GP02"/>
<pin name="AXR011_FSX1_GP03"/>
<pin name="AXR012_FSR1_GP04"/>
<pin name="AXR013_CLKX1_GP05"/>
<pin name="AXR014_CLKR1_GP06"/>
<pin name="AXR015_EPWM0TZ0_ECAP2APWM2_GP07"/>
<pin name="CLKOUT_UHPIHDS2N_GP614"/>
</symbol>
<symbol name="OMAPL138Z-P">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="VDD@31" direction="pwr"/>
<pin name="VDD@32" direction="pwr"/>
<pin name="VDD@33" direction="pwr"/>
<pin name="VDD@34" direction="pwr"/>
<pin name="VDD@35" direction="pwr"/>
<pin name="VDD@36" direction="pwr"/>
<pin name="VDD@37" direction="pwr"/>
<pin name="VDD@38" direction="pwr"/>
<pin name="VDD@39" direction="pwr"/>
<pin name="VDD@40" direction="pwr"/>
<pin name="VDD@41" direction="pwr"/>
<pin name="VDD@42" direction="pwr"/>
<pin name="VDD@43" direction="pwr"/>
<pin name="VDD@44" direction="pwr"/>
<pin name="VDD@45" direction="pwr"/>
<pin name="VDD@46" direction="pwr"/>
<pin name="VDD@47" direction="pwr"/>
<pin name="VDD@48" direction="pwr"/>
<pin name="VDD@49" direction="pwr"/>
<pin name="VDD@50" direction="pwr"/>
<pin name="VDD@51" direction="pwr"/>
<pin name="VDD@52" direction="pwr"/>
<pin name="VDD@53" direction="pwr"/>
<pin name="VDD@54" direction="pwr"/>
<pin name="VDD@55" direction="pwr"/>
<pin name="VDD@56" direction="pwr"/>
<pin name="VDD@57" direction="pwr"/>
<pin name="VDD@58" direction="pwr"/>
<pin name="VDD@59" direction="pwr"/>
<pin name="VDD@60" direction="pwr"/>
<pin name="VDD@61" direction="pwr"/>
<pin name="VDD@62" direction="pwr"/>
<pin name="VDD@63" direction="pwr"/>
<pin name="VDD@64" direction="pwr"/>
<pin name="VDD@65" direction="pwr"/>
<pin name="VDD@66" direction="pwr"/>
<pin name="VDD@67" direction="pwr"/>
<pin name="VDD@68" direction="pwr"/>
<pin name="VDD@69" direction="pwr"/>
<pin name="VDD@70" direction="pwr"/>
<pin name="VDD@71" direction="pwr"/>
<pin name="VDD@72" direction="pwr"/>
<pin name="VDD@73" direction="pwr"/>
<pin name="VDD@74" direction="pwr"/>
<pin name="VDD@75" direction="pwr"/>
<pin name="VDD@76" direction="pwr"/>
<pin name="VDD@77" direction="pwr"/>
<pin name="VDD@78" direction="pwr"/>
<pin name="VDD@79" direction="pwr"/>
<pin name="VDD@80" direction="pwr"/>
<pin name="VDD@81" direction="pwr"/>
<pin name="VDD@82" direction="pwr"/>
<pin name="VDD@83" direction="pwr"/>
<pin name="VDD@84" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
</symbol>
<symbol name="OMAPL138Z-B">
<pin name="DDRA0"/>
<pin name="DDRA1"/>
<pin name="DDRA2"/>
<pin name="DDRA3"/>
<pin name="DDRA4"/>
<pin name="DDRA5"/>
<pin name="DDRA6"/>
<pin name="DDRA7"/>
<pin name="DDRA8"/>
<pin name="DDRA9"/>
<pin name="DDRA10"/>
<pin name="DDRA11"/>
<pin name="DDRA12"/>
<pin name="DDRA13"/>
<pin name="DDRBA0"/>
<pin name="DDRBA1"/>
<pin name="DDRBA2"/>
<pin name="DDRCASN"/>
<pin name="DDRCKE"/>
<pin name="DDRCLKN"/>
<pin name="DDRCLKP"/>
<pin name="DDRCSN"/>
<pin name="DDRD0"/>
<pin name="DDRD1"/>
<pin name="DDRD2"/>
<pin name="DDRD3"/>
<pin name="DDRD4"/>
<pin name="DDRD5"/>
<pin name="DDRD6"/>
<pin name="DDRD7"/>
<pin name="DDRD8"/>
<pin name="DDRD9"/>
<pin name="DDRD10"/>
<pin name="DDRD11"/>
<pin name="DDRD12"/>
<pin name="DDRD13"/>
<pin name="DDRD14"/>
<pin name="DDRD15"/>
<pin name="DDRDQGATE0"/>
<pin name="DDRDQGATE1"/>
<pin name="DDRDQM0N"/>
<pin name="DDRDQM1N"/>
<pin name="DDRDQS0"/>
<pin name="DDRDQS1"/>
<pin name="DDRRASN"/>
<pin name="DDRWEN"/>
</symbol>
<symbol name="OMAPL138Z-C">
<pin name="EMAA0_GP50"/>
<pin name="EMAA1_GP51"/>
<pin name="EMAA2_GP52"/>
<pin name="EMAA3_GP53"/>
<pin name="EMAA4_GP54"/>
<pin name="EMAA5_GP55"/>
<pin name="EMAA6_GP56"/>
<pin name="EMAA7_GP57"/>
<pin name="EMAA8_GP58"/>
<pin name="EMAA9_GP59"/>
<pin name="EMAA10_GP510"/>
<pin name="EMAA11_GP511"/>
<pin name="EMAA12_GP512"/>
<pin name="EMAA13_GP513"/>
<pin name="EMAA14_MMCSD0DAT7_GP514"/>
<pin name="EMAA15_MMCSD0DAT6_GP515"/>
<pin name="EMAA16_MMCSD0DAT5_GP40"/>
<pin name="EMAA17_MMCSD0DAT4_GP41"/>
<pin name="EMAA18_MMCSD0DAT3_GP42"/>
<pin name="EMAA19_MMCSD0DAT2_GP43"/>
<pin name="EMAA20_MMCSD0DAT1_GP44"/>
<pin name="EMAA21_MMCSD0DAT0_GP45"/>
<pin name="EMAA22_MMCSD0CMD_GP46"/>
<pin name="EMAA23_MMCSD0CLK_GP47"/>
<pin name="EMABA0_GP28"/>
<pin name="EMABA1_GP29"/>
<pin name="EMACASN_GP24"/>
<pin name="EMACLK_GP27"/>
<pin name="EMACS0N_GP20"/>
<pin name="EMACS2N_GP315"/>
<pin name="EMACS3N_GP314"/>
<pin name="EMACS4N_GP313"/>
<pin name="EMACS5N_GP212"/>
<pin name="EMAD0_GP48"/>
<pin name="EMAD1_GP49"/>
<pin name="EMAD2_GP410"/>
<pin name="EMAD3_GP411"/>
<pin name="EMAD4_GP412"/>
<pin name="EMAD5_GP413"/>
<pin name="EMAD6_GP414"/>
<pin name="EMAD7_GP415"/>
<pin name="EMAD8_GP30"/>
<pin name="EMAD9_GP31"/>
<pin name="EMAD10_GP32"/>
<pin name="EMAD11_GP33"/>
<pin name="EMAD12_GP34"/>
<pin name="EMAD13_GP35"/>
<pin name="EMAD14_GP36"/>
<pin name="EMAD15_GP37"/>
<pin name="EMAOEN_GP310"/>
<pin name="EMARASN_GP25"/>
<pin name="EMARNW_GP39"/>
<pin name="EMASDCKE_GP26"/>
<pin name="EMAWAIT0_GP38"/>
<pin name="EMAWAIT1_GP21"/>
<pin name="EMAWEDQM0N_GP23"/>
<pin name="EMAWEDQM1N_GP22"/>
<pin name="EMAWEN_GP311"/>
<pin name="EMU0"/>
<pin name="EMU1"/>
</symbol>
<symbol name="OMAPL138Z-D">
<pin name="LCDACENBCSN_GP60"/>
<pin name="MMCSD1CLK_UPPCHBSTART_GP814"/>
<pin name="MMCSD1CMD_UPPCHBENABLE_GP813"/>
<pin name="MMCSD1DAT0_UPPCHBCLOCK_GP815"/>
<pin name="MMCSD1DAT4_LCDVSYNC_GP88"/>
<pin name="MMCSD1DAT5_LCDHSYNC_GP89"/>
<pin name="MMCSD1DAT6_LCDMCLK_GP810"/>
<pin name="MMCSD1DAT7_LCDPCLK_GP811"/>
<pin name="NMIN" direction="in"/>
<pin name="RESETN" direction="in"/>
<pin name="RESETOUTN_UHPIHASN_GP615"/>
<pin name="SATARXN" direction="in"/>
<pin name="SATARXP" direction="in"/>
<pin name="SATATXP" direction="hiz"/>
<pin name="SPI0CLK_EPWM0A_GP18_MIIRXCLK"/>
<pin name="SPI0ENAN_EPWM0B_MIIRXDV"/>
<pin name="SPI0SCS0N_TM64P1OUT12_GP16_MDIOD_TM64P1IN12"/>
<pin name="SPI0SCS1N_TM64P0OUT12_GP17_MDIOCLK_TM64P0IN12"/>
<pin name="SPI0SCS2N_UART0RTS_GP81_MIIRXD0_SATACPDET"/>
<pin name="SPI0SCS3N_UART0CTS_GP82_MIIRXD1_SATAMPSWITCH"/>
<pin name="SPI0SCS4N_UART0TXD_GP83_MIIRXD2"/>
<pin name="SPI0SCS5N_UART0RXD_GP84_MIIRXD3"/>
<pin name="SPI0SIMO_EPWMSYNC0_GP85_MIICRS"/>
<pin name="SPI0SOMI_EPWMSYNCI_GP86_MIIRXER"/>
<pin name="SPI1CLK_GP213"/>
<pin name="SPI1ENAN_GP212"/>
<pin name="SPI1SCS0N_EPWM1B_GP214_TM64P3IN12"/>
<pin name="SPI1SCS1N_EPWM1A_GP215_TM64P2IN12"/>
<pin name="SPI1SCS2N_UART1TXD_SATACPPOD_GP10"/>
<pin name="SPI1SCS3N_UART1RXD_SATALED_GP11"/>
<pin name="SPI1SCS4N_UART2TXD_I2C1SDA_GP12"/>
<pin name="SPI1SCS5N_UART2RXD_I2C1SCL_GP13"/>
<pin name="SPI1SCS6N_I2C0SDA_TM64P3OUT12_GP14"/>
<pin name="SPI1SCS7N_I2C0SCL_TM64P2OUT12_GP15"/>
<pin name="SPI1SIMO_GP210"/>
<pin name="SPI1SOMI_GP211"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRSTN" direction="in"/>
<pin name="UHPIHCNTL0_UPPCHACLOCK_GP611"/>
<pin name="UHPIHCNTL1_UPPCHASTART_GP610"/>
<pin name="UHPIHHWIL_UPPCHAENABLE_GP69"/>
<pin name="UHPIHINTN_GP612"/>
<pin name="UHPIHRDYN_GP613"/>
<pin name="UHPIHRWN_UPPCHAWAIT_GP68"/>
<pin name="UPPCHBWAIT_GP812"/>
<pin name="USB0DRVVBUS"/>
</symbol>
<symbol name="OMAPL138Z-E">
<pin name="VPIFCLKIN0_UHPIHCSN_GP67_UPP2XTXCLK"/>
<pin name="VPIFCLKIN1_UHPIHDS1N_GP66"/>
<pin name="VPIFCLKIN2_MMCSD1DAT3_GP64"/>
<pin name="VPIFCLKIN3_MMCSD1DAT1_GP62"/>
<pin name="VPIFCLKO2_MMCSD1DAT2_GP63"/>
<pin name="VPIFCLKO3_GP61"/>
<pin name="VPIFDIN0_UHPIHD8_UPPD8_RMIICRSDV"/>
<pin name="VPIFDIN1_UHPIHD9_UPPD9_RMIIMHZ50CLK"/>
<pin name="VPIFDIN2_UHPIHD10_UPPD10_RMIIRXER"/>
<pin name="VPIFDIN3_UHPIHD11_UPPD11_RMIIRXD0"/>
<pin name="VPIFDIN4_UHPIHD12_UPPD12_RMIIRXD1"/>
<pin name="VPIFDIN5_UHPIHD13_UPPD13_RMIITXEN"/>
<pin name="VPIFDIN6_UHPIHD14_UPPD14_RMIITXD0"/>
<pin name="VPIFDIN7_UHPIHD15_UPPD15_RMIITXD1"/>
<pin name="VPIFDIN8_UHPIHD0_UPPD0_GP65"/>
<pin name="VPIFDIN9_UHPIHD1_UPPD1"/>
<pin name="VPIFDIN10_UHPIHD2_UPPD2"/>
<pin name="VPIFDIN11_UHPIHD3_UPPD3"/>
<pin name="VPIFDIN12_UHPIHD4_UPPD4"/>
<pin name="VPIFDIN13FIELD_UHPIHD5_UPPD5"/>
<pin name="VPIFDIN14HSYNC_UHPIHD6_UPPD6"/>
<pin name="VPIFDIN15VSYNC_UHPIHD7_UPPD7"/>
<pin name="VPIFDOUT0_LCDD0_UPPXD8_GP78"/>
<pin name="VPIFDOUT1_LCDD1_UPPXD9_GP79"/>
<pin name="VPIFDOUT2_LCDD2_UPPXD10_GP710"/>
<pin name="VPIFDOUT3_LCDD3_UPPXD11_GP711"/>
<pin name="VPIFDOUT4_LCDD4_UPPXD12_GP712"/>
<pin name="VPIFDOUT5_LCDD5_UPPXD13_GP713"/>
<pin name="VPIFDOUT6_LCDD6_UPPXD14_GP714"/>
<pin name="VPIFDOUT7_LCDD7_UPPXD15_GP715"/>
<pin name="VPIFDOUT8_LCDD8_UPPXD0_GP70_BOOT0"/>
<pin name="VPIFDOUT9_LCDD9_UPPXD1_GP71_BOOT1"/>
<pin name="VPIFDOUT10_LCDD10_UPPXD2_GP72_BOOT2"/>
<pin name="VPIFDOUT11_LCDD11_UPPXD3_GP73_BOOT3"/>
<pin name="VPIFDOUT12_LCDD12_UPPXD4_GP74_BOOT4"/>
<pin name="VPIFDOUT13_LCDD13_UPPXD5_GP75_BOOT5"/>
<pin name="VPIFDOUT14_LCDD14_UPPXD6_GP76_BOOT6"/>
<pin name="VPIFDOUT15_LCDD15_UPPXD7_GP77_BOOT7"/>
</symbol>
<symbol name="OMAP-L138_ZCE-P">
<pin name="VDD@1" direction="pwr"/>
<pin name="VDD@2" direction="pwr"/>
<pin name="VDD@3" direction="pwr"/>
<pin name="VDD@4" direction="pwr"/>
<pin name="VDD@5" direction="pwr"/>
<pin name="VDD@6" direction="pwr"/>
<pin name="VDD@7" direction="pwr"/>
<pin name="VDD@8" direction="pwr"/>
<pin name="VDD@9" direction="pwr"/>
<pin name="VDD@10" direction="pwr"/>
<pin name="VDD@11" direction="pwr"/>
<pin name="VDD@12" direction="pwr"/>
<pin name="VDD@13" direction="pwr"/>
<pin name="VDD@14" direction="pwr"/>
<pin name="VDD@15" direction="pwr"/>
<pin name="VDD@16" direction="pwr"/>
<pin name="VDD@17" direction="pwr"/>
<pin name="VDD@18" direction="pwr"/>
<pin name="VDD@19" direction="pwr"/>
<pin name="VDD@20" direction="pwr"/>
<pin name="VDD@21" direction="pwr"/>
<pin name="VDD@22" direction="pwr"/>
<pin name="VDD@23" direction="pwr"/>
<pin name="VDD@24" direction="pwr"/>
<pin name="VDD@25" direction="pwr"/>
<pin name="VDD@26" direction="pwr"/>
<pin name="VDD@27" direction="pwr"/>
<pin name="VDD@28" direction="pwr"/>
<pin name="VDD@29" direction="pwr"/>
<pin name="VDD@30" direction="pwr"/>
<pin name="VDD@31" direction="pwr"/>
<pin name="VDD@32" direction="pwr"/>
<pin name="VDD@33" direction="pwr"/>
<pin name="VDD@34" direction="pwr"/>
<pin name="VDD@35" direction="pwr"/>
<pin name="VDD@36" direction="pwr"/>
<pin name="VDD@37" direction="pwr"/>
<pin name="VDD@38" direction="pwr"/>
<pin name="VDD@39" direction="pwr"/>
<pin name="VDD@40" direction="pwr"/>
<pin name="VDD@41" direction="pwr"/>
<pin name="VDD@42" direction="pwr"/>
<pin name="VDD@43" direction="pwr"/>
<pin name="VDD@44" direction="pwr"/>
<pin name="VDD@45" direction="pwr"/>
<pin name="VDD@46" direction="pwr"/>
<pin name="VDD@47" direction="pwr"/>
<pin name="VDD@48" direction="pwr"/>
<pin name="VDD@49" direction="pwr"/>
<pin name="VDD@50" direction="pwr"/>
<pin name="VDD@51" direction="pwr"/>
<pin name="VDD@52" direction="pwr"/>
<pin name="VDD@53" direction="pwr"/>
<pin name="VDD@54" direction="pwr"/>
<pin name="VDD@55" direction="pwr"/>
<pin name="VDD@56" direction="pwr"/>
<pin name="VDD@57" direction="pwr"/>
<pin name="VDD@58" direction="pwr"/>
<pin name="VDD@59" direction="pwr"/>
<pin name="VDD@60" direction="pwr"/>
<pin name="VDD@61" direction="pwr"/>
<pin name="VDD@62" direction="pwr"/>
<pin name="VDD@63" direction="pwr"/>
<pin name="VDD@64" direction="pwr"/>
<pin name="VDD@65" direction="pwr"/>
<pin name="VDD@66" direction="pwr"/>
<pin name="VDD@67" direction="pwr"/>
<pin name="VDD@68" direction="pwr"/>
<pin name="VDD@69" direction="pwr"/>
<pin name="VDD@70" direction="pwr"/>
<pin name="VDD@71" direction="pwr"/>
<pin name="VDD@72" direction="pwr"/>
<pin name="VDD@73" direction="pwr"/>
<pin name="VDD@74" direction="pwr"/>
<pin name="VDD@75" direction="pwr"/>
<pin name="VDD@76" direction="pwr"/>
<pin name="VDD@77" direction="pwr"/>
<pin name="VDD@78" direction="pwr"/>
<pin name="VDD@79" direction="pwr"/>
<pin name="VDD@80" direction="pwr"/>
<pin name="VDD@81" direction="pwr"/>
<pin name="VDD@82" direction="pwr"/>
<pin name="VDD@83" direction="pwr"/>
<pin name="VDD@84" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
</symbol>
<symbol name="OMAP-L138_ZCE-A">
<pin name="ACLKR_GP015"/>
<pin name="ACLKX_GP014"/>
<pin name="AFSR0_GP013"/>
<pin name="AFSX0_GP012"/>
<pin name="AHCLKR_UART1RTS_GP011"/>
<pin name="AHCLKX_USBREFCLKIN_UART1CTS_GP010"/>
<pin name="AMUTEIN_RTCALARM_UART2CTS_GP08_DEEPSLEEPN"/>
<pin name="AMUTE_UART2RTS_GP09"/>
<pin name="AXR00_ECAP0APWM0_GP87_MIITXD0_CLKS0"/>
<pin name="AXR01_DX0_GP19MIITXD1"/>
<pin name="AXR02_DR0_GP110_MIITXD2"/>
<pin name="AXR03_FSX0_GP111_MIITXD3"/>
<pin name="AXR04_FSR0_GP112_MIICOL"/>
<pin name="AXR05_CLKX0_GP113_MIITXCLK"/>
<pin name="AXR06_CLKR0_GP114_MIITXEN"/>
<pin name="AXR07_EPWM1TZ0_GP115"/>
<pin name="AXR08_CLKS1_ECAP1APWM1_GP00"/>
<pin name="AXR09_DX1_GP01"/>
<pin name="AXR010_DR1_GP02"/>
<pin name="AXR011_FSX1_GP03"/>
<pin name="AXR012_FSR1_GP04"/>
<pin name="AXR013_CLKX1_GP05"/>
<pin name="AXR014_CLKR1_GP06"/>
<pin name="AXR015_EPWM0TZ0_ECAP2APWM2_GP07"/>
<pin name="CLKOUT_UHPIHDS2N_GP614"/>
</symbol>
<symbol name="OMAP-L138_ZCE-B">
<pin name="DDRA0"/>
<pin name="DDRA1"/>
<pin name="DDRA2"/>
<pin name="DDRA3"/>
<pin name="DDRA4"/>
<pin name="DDRA5"/>
<pin name="DDRA6"/>
<pin name="DDRA7"/>
<pin name="DDRA8"/>
<pin name="DDRA9"/>
<pin name="DDRA10"/>
<pin name="DDRA11"/>
<pin name="DDRA12"/>
<pin name="DDRA13"/>
<pin name="DDRBA0"/>
<pin name="DDRBA1"/>
<pin name="DDRBA2"/>
<pin name="DDRCASN"/>
<pin name="DDRCKE"/>
<pin name="DDRCLKN"/>
<pin name="DDRCLKP"/>
<pin name="DDRCSN"/>
<pin name="DDRD0"/>
<pin name="DDRD1"/>
<pin name="DDRD2"/>
<pin name="DDRD3"/>
<pin name="DDRD4"/>
<pin name="DDRD5"/>
<pin name="DDRD6"/>
<pin name="DDRD7"/>
<pin name="DDRD8"/>
<pin name="DDRD9"/>
<pin name="DDRD10"/>
<pin name="DDRD11"/>
<pin name="DDRD12"/>
<pin name="DDRD13"/>
<pin name="DDRD14"/>
<pin name="DDRD15"/>
<pin name="DDRDQGATE0"/>
<pin name="DDRDQGATE1"/>
<pin name="DDRDQM0N"/>
<pin name="DDRDQM1N"/>
<pin name="DDRDQS0"/>
<pin name="DDRDQS1"/>
<pin name="DDRRASN"/>
<pin name="DDRWEN"/>
</symbol>
<symbol name="OMAP-L138_ZCE-C">
<pin name="EMAA0_GP50"/>
<pin name="EMAA1_GP51"/>
<pin name="EMAA2_GP52"/>
<pin name="EMAA3_GP53"/>
<pin name="EMAA4_GP54"/>
<pin name="EMAA5_GP55"/>
<pin name="EMAA6_GP56"/>
<pin name="EMAA7_GP57"/>
<pin name="EMAA8_GP58"/>
<pin name="EMAA9_GP59"/>
<pin name="EMAA10_GP510"/>
<pin name="EMAA11_GP511"/>
<pin name="EMAA12_GP512"/>
<pin name="EMAA13_GP513"/>
<pin name="EMAA14_MMCSD0DAT7_GP514"/>
<pin name="EMAA15_MMCSD0DAT6_GP515"/>
<pin name="EMAA16_MMCSD0DAT5_GP40"/>
<pin name="EMAA17_MMCSD0DAT4_GP41"/>
<pin name="EMAA18_MMCSD0DAT3_GP42"/>
<pin name="EMAA19_MMCSD0DAT2_GP43"/>
<pin name="EMAA20_MMCSD0DAT1_GP44"/>
<pin name="EMAA21_MMCSD0DAT0_GP45"/>
<pin name="EMAA22_MMCSD0CMD_GP46"/>
<pin name="EMAA23_MMCSD0CLK_GP47"/>
<pin name="EMABA0_GP28"/>
<pin name="EMABA1_GP29"/>
<pin name="EMACASN_GP24"/>
<pin name="EMACLK_GP27"/>
<pin name="EMACS0N_GP20"/>
<pin name="EMACS2N_GP315"/>
<pin name="EMACS3N_GP314"/>
<pin name="EMACS4N_GP313"/>
<pin name="EMACS5N_GP212"/>
<pin name="EMAD0_GP48"/>
<pin name="EMAD1_GP49"/>
<pin name="EMAD2_GP410"/>
<pin name="EMAD3_GP411"/>
<pin name="EMAD4_GP412"/>
<pin name="EMAD5_GP413"/>
<pin name="EMAD6_GP414"/>
<pin name="EMAD7_GP415"/>
<pin name="EMAD8_GP30"/>
<pin name="EMAD9_GP31"/>
<pin name="EMAD10_GP32"/>
<pin name="EMAD11_GP33"/>
<pin name="EMAD12_GP34"/>
<pin name="EMAD13_GP35"/>
<pin name="EMAD14_GP36"/>
<pin name="EMAD15_GP37"/>
<pin name="EMAOEN_GP310"/>
<pin name="EMARASN_GP25"/>
<pin name="EMARNW_GP39"/>
<pin name="EMASDCKE_GP26"/>
<pin name="EMAWAIT0_GP38"/>
<pin name="EMAWAIT1_GP21"/>
<pin name="EMAWEDQM0N_GP23"/>
<pin name="EMAWEDQM1N_GP22"/>
<pin name="EMAWEN_GP311"/>
<pin name="EMU0"/>
<pin name="EMU1"/>
</symbol>
<symbol name="OMAP-L138_ZCE-D">
<pin name="LCDACENBCSN_GP60"/>
<pin name="MMCSD1CLK_UPPCHBSTART_GP814"/>
<pin name="MMCSD1CMD_UPPCHBENABLE_GP813"/>
<pin name="MMCSD1DAT0_UPPCHBCLOCK_GP815"/>
<pin name="MMCSD1DAT4_LCDVSYNC_GP88"/>
<pin name="MMCSD1DAT5_LCDHSYNC_GP89"/>
<pin name="MMCSD1DAT6_LCDMCLK_GP810"/>
<pin name="MMCSD1DAT7_LCDPCLK_GP811"/>
<pin name="NMIN" direction="in"/>
<pin name="RESETN" direction="in"/>
<pin name="RESETOUTN_UHPIHASN_GP615"/>
<pin name="SATARXN" direction="in"/>
<pin name="SATARXP" direction="in"/>
<pin name="SATATXP" direction="hiz"/>
<pin name="SPI0CLK_EPWM0A_GP18_MIIRXCLK"/>
<pin name="SPI0ENAN_EPWM0B_MIIRXDV"/>
<pin name="SPI0SCS0N_TM64P1OUT12_GP16_MDIOD_TM64P1IN12"/>
<pin name="SPI0SCS1N_TM64P0OUT12_GP17_MDIOCLK_TM64P0IN12"/>
<pin name="SPI0SCS2N_UART0RTS_GP81_MIIRXD0_SATACPDET"/>
<pin name="SPI0SCS3N_UART0CTS_GP82_MIIRXD1_SATAMPSWITCH"/>
<pin name="SPI0SCS4N_UART0TXD_GP83_MIIRXD2"/>
<pin name="SPI0SCS5N_UART0RXD_GP84_MIIRXD3"/>
<pin name="SPI0SIMO_EPWMSYNC0_GP85_MIICRS"/>
<pin name="SPI0SOMI_EPWMSYNCI_GP86_MIIRXER"/>
<pin name="SPI1CLK_GP213"/>
<pin name="SPI1ENAN_GP212"/>
<pin name="SPI1SCS0N_EPWM1B_GP214_TM64P3IN12"/>
<pin name="SPI1SCS1N_EPWM1A_GP215_TM64P2IN12"/>
<pin name="SPI1SCS2N_UART1TXD_SATACPPOD_GP10"/>
<pin name="SPI1SCS3N_UART1RXD_SATALED_GP11"/>
<pin name="SPI1SCS4N_UART2TXD_I2C1SDA_GP12"/>
<pin name="SPI1SCS5N_UART2RXD_I2C1SCL_GP13"/>
<pin name="SPI1SCS6N_I2C0SDA_TM64P3OUT12_GP14"/>
<pin name="SPI1SCS7N_I2C0SCL_TM64P2OUT12_GP15"/>
<pin name="SPI1SIMO_GP210"/>
<pin name="SPI1SOMI_GP211"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TMS" direction="in"/>
<pin name="TRSTN" direction="in"/>
<pin name="UHPIHCNTL0_UPPCHACLOCK_GP611"/>
<pin name="UHPIHCNTL1_UPPCHASTART_GP610"/>
<pin name="UHPIHHWIL_UPPCHAENABLE_GP69"/>
<pin name="UHPIHINTN_GP612"/>
<pin name="UHPIHRDYN_GP613"/>
<pin name="UHPIHRWN_UPPCHAWAIT_GP68"/>
<pin name="UPPCHBWAIT_GP812"/>
<pin name="USB0DRVVBUS"/>
</symbol>
<symbol name="OMAP-L138_ZCE-E">
<pin name="VPIFCLKIN0_UHPIHCSN_GP67_UPP2XTXCLK"/>
<pin name="VPIFCLKIN1_UHPIHDS1N_GP66"/>
<pin name="VPIFCLKIN2_MMCSD1DAT3_GP64"/>
<pin name="VPIFCLKIN3_MMCSD1DAT1_GP62"/>
<pin name="VPIFCLKO2_MMCSD1DAT2_GP63"/>
<pin name="VPIFCLKO3_GP61"/>
<pin name="VPIFDIN0_UHPIHD8_UPPD8_RMIICRSDV"/>
<pin name="VPIFDIN1_UHPIHD9_UPPD9_RMIIMHZ50CLK"/>
<pin name="VPIFDIN2_UHPIHD10_UPPD10_RMIIRXER"/>
<pin name="VPIFDIN3_UHPIHD11_UPPD11_RMIIRXD0"/>
<pin name="VPIFDIN4_UHPIHD12_UPPD12_RMIIRXD1"/>
<pin name="VPIFDIN5_UHPIHD13_UPPD13_RMIITXEN"/>
<pin name="VPIFDIN6_UHPIHD14_UPPD14_RMIITXD0"/>
<pin name="VPIFDIN7_UHPIHD15_UPPD15_RMIITXD1"/>
<pin name="VPIFDIN8_UHPIHD0_UPPD0_GP65"/>
<pin name="VPIFDIN9_UHPIHD1_UPPD1"/>
<pin name="VPIFDIN10_UHPIHD2_UPPD2"/>
<pin name="VPIFDIN11_UHPIHD3_UPPD3"/>
<pin name="VPIFDIN12_UHPIHD4_UPPD4"/>
<pin name="VPIFDIN13FIELD_UHPIHD5_UPPD5"/>
<pin name="VPIFDIN14HSYNC_UHPIHD6_UPPD6"/>
<pin name="VPIFDIN15VSYNC_UHPIHD7_UPPD7"/>
<pin name="VPIFDOUT0_LCDD0_UPPXD8_GP78"/>
<pin name="VPIFDOUT1_LCDD1_UPPXD9_GP79"/>
<pin name="VPIFDOUT2_LCDD2_UPPXD10_GP710"/>
<pin name="VPIFDOUT3_LCDD3_UPPXD11_GP711"/>
<pin name="VPIFDOUT4_LCDD4_UPPXD12_GP712"/>
<pin name="VPIFDOUT5_LCDD5_UPPXD13_GP713"/>
<pin name="VPIFDOUT6_LCDD6_UPPXD14_GP714"/>
<pin name="VPIFDOUT7_LCDD7_UPPXD15_GP715"/>
<pin name="VPIFDOUT8_LCDD8_UPPXD0_GP70_BOOT0"/>
<pin name="VPIFDOUT9_LCDD9_UPPXD1_GP71_BOOT1"/>
<pin name="VPIFDOUT10_LCDD10_UPPXD2_GP72_BOOT2"/>
<pin name="VPIFDOUT11_LCDD11_UPPXD3_GP73_BOOT3"/>
<pin name="VPIFDOUT12_LCDD12_UPPXD4_GP74_BOOT4"/>
<pin name="VPIFDOUT13_LCDD13_UPPXD5_GP75_BOOT5"/>
<pin name="VPIFDOUT14_LCDD14_UPPXD6_GP76_BOOT6"/>
<pin name="VPIFDOUT15_LCDD15_UPPXD7_GP77_BOOT7"/>
</symbol>
<symbol name="TMS320VC5509A">
<pin name="A0"/>
<pin name="A0E" direction="out"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
<pin name="ADVDD" direction="pwr"/>
<pin name="ADVSS" direction="pwr"/>
<pin name="AIN0" direction="pas"/>
<pin name="AIN1" direction="pas"/>
<pin name="AIN2" direction="pas"/>
<pin name="AIN3" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS@1" direction="pwr"/>
<pin name="AVSS@2" direction="pwr"/>
<pin name="C0"/>
<pin name="C1" direction="out"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="C4"/>
<pin name="C5"/>
<pin name="C6"/>
<pin name="C7"/>
<pin name="C8"/>
<pin name="C9"/>
<pin name="C10"/>
<pin name="C11"/>
<pin name="C12"/>
<pin name="C13"/>
<pin name="C14"/>
<pin name="CLKOUT" direction="out"/>
<pin name="CLKR0"/>
<pin name="CLKX0"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="CVDD@7" direction="pwr"/>
<pin name="CVDD@8" direction="pwr"/>
<pin name="CVDD@9" direction="pwr"/>
<pin name="CVDD@10" direction="pwr"/>
<pin name="CVDD@11" direction="pwr"/>
<pin name="CVDD@12" direction="pwr"/>
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="DN" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="DR0" direction="in"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="DVDD@7" direction="pwr"/>
<pin name="DVDD@8" direction="pwr"/>
<pin name="DVDD@9" direction="pwr"/>
<pin name="DVDD@10" direction="pwr"/>
<pin name="DVDD@11" direction="pwr"/>
<pin name="DVDD@12" direction="pwr"/>
<pin name="DVDD@13" direction="pwr"/>
<pin name="DVDD@14" direction="pwr"/>
<pin name="DVDD@15" direction="pwr"/>
<pin name="DVDD@16" direction="pwr"/>
<pin name="DX0" direction="out"/>
<pin name="EMU0" direction="in"/>
<pin name="EMU1" direction="in"/>
<pin name="FSR0"/>
<pin name="FSX0"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NINT0" direction="in"/>
<pin name="NINT1" direction="in"/>
<pin name="NINT2" direction="in"/>
<pin name="NINT3" direction="in"/>
<pin name="NINT4" direction="in"/>
<pin name="NRESET" direction="in"/>
<pin name="PU" direction="pas"/>
<pin name="RCVDD" direction="pwr"/>
<pin name="RDVDD@1" direction="pwr"/>
<pin name="RDVDD@2" direction="pwr"/>
<pin name="RDVDD@3" direction="pwr"/>
<pin name="RTCINX1" direction="pas"/>
<pin name="RTCINX2" direction="pas"/>
<pin name="RVDD@1" direction="pwr"/>
<pin name="RVDD@2" direction="pwr"/>
<pin name="RVDD@3" direction="pwr"/>
<pin name="S10"/>
<pin name="S11"/>
<pin name="S12"/>
<pin name="S13"/>
<pin name="S14"/>
<pin name="S15"/>
<pin name="S20"/>
<pin name="S21"/>
<pin name="S22"/>
<pin name="S23"/>
<pin name="S24"/>
<pin name="S25"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TINOUT0"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="USBPLLVDD" direction="pwr"/>
<pin name="USBPLLVSS" direction="pwr"/>
<pin name="USBVDD" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="X1" direction="pas"/>
<pin name="X2CLKIN" direction="in"/>
<pin name="XF" direction="out"/>
</symbol>
<symbol name="TMS320VC5509-A">
<pin name="A0"/>
<pin name="A0E" direction="out"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="A3"/>
<pin name="A4"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="A9"/>
<pin name="A10"/>
<pin name="A11"/>
<pin name="A12"/>
<pin name="A13"/>
<pin name="A14"/>
<pin name="A15"/>
<pin name="A16" direction="out"/>
<pin name="A17" direction="out"/>
<pin name="A18" direction="out"/>
<pin name="A19" direction="out"/>
<pin name="A20" direction="out"/>
</symbol>
<symbol name="TMS320VC5509-B">
<pin name="C0"/>
<pin name="C1" direction="out"/>
<pin name="C2"/>
<pin name="C3"/>
<pin name="C4"/>
<pin name="C5"/>
<pin name="C6"/>
<pin name="C7"/>
<pin name="C8"/>
<pin name="C9"/>
<pin name="C10"/>
<pin name="C11"/>
<pin name="C12"/>
<pin name="C13"/>
<pin name="C14"/>
<pin name="CLKOUT" direction="out"/>
<pin name="CLKR0"/>
<pin name="CLKX0"/>
</symbol>
<symbol name="TMS320VC5509-C">
<pin name="D0"/>
<pin name="D1"/>
<pin name="D2"/>
<pin name="D3"/>
<pin name="D4"/>
<pin name="D5"/>
<pin name="D6"/>
<pin name="D7"/>
<pin name="D8"/>
<pin name="D9"/>
<pin name="D10"/>
<pin name="D11"/>
<pin name="D12"/>
<pin name="D13"/>
<pin name="D14"/>
<pin name="D15"/>
<pin name="DN" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="DR0" direction="in"/>
</symbol>
<symbol name="TMS320VC5509-D">
<pin name="DX0" direction="out"/>
<pin name="EMU0" direction="in"/>
<pin name="EMU1" direction="in"/>
<pin name="FSR0"/>
<pin name="FSX0"/>
<pin name="GPIO0"/>
<pin name="GPIO1"/>
<pin name="GPIO2"/>
<pin name="GPIO3"/>
<pin name="GPIO4"/>
<pin name="GPIO5"/>
<pin name="GPIO6"/>
<pin name="GPIO7"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NINT0" direction="in"/>
<pin name="NINT1" direction="in"/>
<pin name="NINT2" direction="in"/>
<pin name="NINT3" direction="in"/>
<pin name="NINT4" direction="in"/>
<pin name="NRESET" direction="in"/>
<pin name="PU" direction="pas"/>
<pin name="RTCINX1" direction="pas"/>
<pin name="RTCINX2" direction="pas"/>
<pin name="ADVDD" direction="pwr"/>
<pin name="ADVSS" direction="pwr"/>
<pin name="AIN0" direction="pas"/>
<pin name="AIN1" direction="pas"/>
<pin name="AIN2" direction="pas"/>
<pin name="AIN3" direction="pas"/>
<pin name="AVDD" direction="pwr"/>
<pin name="AVSS@1" direction="pwr"/>
<pin name="AVSS@2" direction="pwr"/>
</symbol>
<symbol name="TMS320VC5509-E">
<pin name="S10"/>
<pin name="S11"/>
<pin name="S12"/>
<pin name="S13"/>
<pin name="S14"/>
<pin name="S15"/>
<pin name="S20"/>
<pin name="S21"/>
<pin name="S22"/>
<pin name="S23"/>
<pin name="S24"/>
<pin name="S25"/>
<pin name="SCL"/>
<pin name="SDA"/>
<pin name="TCK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="TINOUT0"/>
<pin name="TMS" direction="in"/>
<pin name="TRST" direction="in"/>
<pin name="USBPLLVDD" direction="pwr"/>
<pin name="USBPLLVSS" direction="pwr"/>
<pin name="USBVDD" direction="pwr"/>
<pin name="X1" direction="pas"/>
<pin name="X2CLKIN" direction="in"/>
<pin name="XF" direction="out"/>
</symbol>
<symbol name="TMS320VC5509-P">
<pin name="CVDD@1" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="CVDD@7" direction="pwr"/>
<pin name="CVDD@8" direction="pwr"/>
<pin name="CVDD@9" direction="pwr"/>
<pin name="CVDD@10" direction="pwr"/>
<pin name="CVDD@11" direction="pwr"/>
<pin name="CVDD@12" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="DVDD@7" direction="pwr"/>
<pin name="DVDD@8" direction="pwr"/>
<pin name="DVDD@9" direction="pwr"/>
<pin name="DVDD@10" direction="pwr"/>
<pin name="DVDD@11" direction="pwr"/>
<pin name="DVDD@12" direction="pwr"/>
<pin name="DVDD@13" direction="pwr"/>
<pin name="DVDD@14" direction="pwr"/>
<pin name="DVDD@15" direction="pwr"/>
<pin name="DVDD@16" direction="pwr"/>
<pin name="RCVDD" direction="pwr"/>
<pin name="RDVDD@1" direction="pwr"/>
<pin name="RDVDD@2" direction="pwr"/>
<pin name="RDVDD@3" direction="pwr"/>
<pin name="RVDD@1" direction="pwr"/>
<pin name="RVDD@2" direction="pwr"/>
<pin name="RVDD@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
</symbol>
<symbol name="TUSB2046B">
<pin name="DP0"/>
<pin name="DM0"/>
<pin name="VCC" direction="pwr"/>
<pin name="!RESET" direction="in"/>
<pin name="EECLK" direction="out"/>
<pin name="EEDATA/GANGED"/>
<pin name="GND" direction="pwr"/>
<pin name="BUSPWR" direction="in"/>
<pin name="!PWRON1" direction="out"/>
<pin name="!OVRCUR1" direction="in"/>
<pin name="DM1"/>
<pin name="DP1"/>
<pin name="!PWRON2" direction="out"/>
<pin name="!OVRCUR2" direction="in"/>
<pin name="DM2"/>
<pin name="DP2"/>
<pin name="!PWRON3" direction="out"/>
<pin name="!OVRCUR3" direction="in"/>
<pin name="DM3"/>
<pin name="DP3"/>
<pin name="!PWRON4" direction="out"/>
<pin name="!OVRCUR4" direction="in"/>
<pin name="DM4"/>
<pin name="DP4"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="!EXTMEM" direction="in"/>
<pin name="TSTPLL/48MCLK"/>
<pin name="GND@1" direction="pwr"/>
<pin name="XTAL2" direction="out"/>
<pin name="XTAL1" direction="in"/>
<pin name="TSTMODE" direction="in"/>
<pin name="SUSPND" direction="out"/>
</symbol>
<symbol name="EXP10">
<pin name="EXP" direction="pas"/>
<pin name="EXP@1" direction="pas"/>
<pin name="EXP@2" direction="pas"/>
<pin name="EXP@3" direction="pas"/>
<pin name="EXP@4" direction="pas"/>
<pin name="EXP@5" direction="pas"/>
<pin name="EXP@6" direction="pas"/>
<pin name="EXP@7" direction="pas"/>
<pin name="EXP@8" direction="pas"/>
<pin name="EXP@9" direction="pas"/>
</symbol>
<symbol name="SN74LVCR162245A">
<pin name="1DIR" direction="in"/>
<pin name="1B1" direction="hiz"/>
<pin name="1B2" direction="hiz"/>
<pin name="GND" direction="pwr"/>
<pin name="1B3" direction="hiz"/>
<pin name="1B4" direction="hiz"/>
<pin name="VCC" direction="pwr"/>
<pin name="1B5" direction="hiz"/>
<pin name="1B6" direction="hiz"/>
<pin name="GND@1" direction="pwr"/>
<pin name="1B7" direction="hiz"/>
<pin name="1B8" direction="hiz"/>
<pin name="2B1" direction="hiz"/>
<pin name="2B2" direction="hiz"/>
<pin name="GND@2" direction="pwr"/>
<pin name="2B3" direction="hiz"/>
<pin name="2B4" direction="hiz"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="2B5" direction="hiz"/>
<pin name="2B6" direction="hiz"/>
<pin name="GND@3" direction="hiz"/>
<pin name="2B7" direction="hiz"/>
<pin name="2B8" direction="hiz"/>
<pin name="2DIR" direction="in"/>
<pin name="2!OE" direction="in"/>
<pin name="2A8" direction="hiz"/>
<pin name="2A7" direction="hiz"/>
<pin name="GND@4" direction="pwr"/>
<pin name="2A6" direction="hiz"/>
<pin name="2A5" direction="hiz"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="2A4" direction="hiz"/>
<pin name="2A3" direction="hiz"/>
<pin name="GND@5" direction="pwr"/>
<pin name="2A2" direction="hiz"/>
<pin name="2A1" direction="hiz"/>
<pin name="1A8" direction="hiz"/>
<pin name="1A7" direction="hiz"/>
<pin name="GND@6" direction="hiz"/>
<pin name="1A6" direction="hiz"/>
<pin name="1A5" direction="hiz"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="1A4" direction="hiz"/>
<pin name="1A3" direction="hiz"/>
<pin name="GND@7" direction="pwr"/>
<pin name="1A2" direction="hiz"/>
<pin name="1A1" direction="hiz"/>
<pin name="1!OE" direction="in"/>
</symbol>
<symbol name="MSP430F23X">
<pin name="DVCC" direction="pwr"/>
<pin name="P6_3/A3"/>
<pin name="P6_4/A4"/>
<pin name="P6_5/A5"/>
<pin name="P6_6/A6"/>
<pin name="P6_7/A7/SVSIN"/>
<pin name="VREF+" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="VEREF+" direction="in"/>
<pin name="VREF--/VEREF--" direction="in"/>
<pin name="P1_0/TACLK/CAOUT"/>
<pin name="P1_1/TA0"/>
<pin name="P1_2/TA1"/>
<pin name="P1_3/TA2"/>
<pin name="P1_4/SMCLK"/>
<pin name="P1_5/TA0"/>
<pin name="P1_6/TA1"/>
<pin name="P1_7/TA2"/>
<pin name="P2_0/ACLK/CA2"/>
<pin name="P2_1/TAINCLK/CA3"/>
<pin name="P2_2/CAOUT/TA0/CA4"/>
<pin name="P2_3/CA0/TA1"/>
<pin name="P2_4/CA1/TA2"/>
<pin name="P2_5/ROSC/CA5"/>
<pin name="P2_6/ADC12CLK/CA6"/>
<pin name="P2_7/TA0/CA7"/>
<pin name="P3_0/UCB0STE/UCA0CLK"/>
<pin name="P3_1/UCB0SIMO/UCB0SDA"/>
<pin name="P3_2/UCB0SOMI/UCB0SCL"/>
<pin name="P3_3/UCB0CLK/UCA0STE"/>
<pin name="P3_4/UCA0TXD/UCA0SIMO"/>
<pin name="P3_5/UCA0RXD/UCA0SOMI"/>
<pin name="P3_6"/>
<pin name="P3_7"/>
<pin name="P4_0/TB0"/>
<pin name="P4_1/TB1"/>
<pin name="P4_2/TB2"/>
<pin name="P4_3"/>
<pin name="P4_4"/>
<pin name="P4_5"/>
<pin name="P4_6"/>
<pin name="P4_7/TBCLK"/>
<pin name="P5_0"/>
<pin name="P5_1"/>
<pin name="P5_2"/>
<pin name="P5_3"/>
<pin name="P5_4/MCLK"/>
<pin name="P5_5/SMCLK"/>
<pin name="P5_6/ACLK"/>
<pin name="P5_7/TBOUTH/SVSOUT"/>
<pin name="XT2OUT" direction="out"/>
<pin name="XT2IN" direction="in"/>
<pin name="TDO/TDI"/>
<pin name="TDI/TCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="!RST!/NMI" direction="in"/>
<pin name="P6_0/A0"/>
<pin name="P6_1/A1"/>
<pin name="P6_2/A2"/>
<pin name="AVSS" direction="pwr"/>
<pin name="DVSS" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="MSP430F24X">
<pin name="DVCC" direction="pwr"/>
<pin name="P6_3/A3"/>
<pin name="P6_4/A4"/>
<pin name="P6_5/A5"/>
<pin name="P6_6/A6"/>
<pin name="P6_7/A7/SVSIN"/>
<pin name="VREF+" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="VEREF+" direction="in"/>
<pin name="VREF--/VEREF--" direction="in"/>
<pin name="P1_0/TACLK/CAOUT"/>
<pin name="P1_1/TA0"/>
<pin name="P1_2/TA1"/>
<pin name="P1_3/TA2"/>
<pin name="P1_4/SMCLK"/>
<pin name="P1_5/TA0"/>
<pin name="P1_6/TA1"/>
<pin name="P1_7/TA2"/>
<pin name="P2_0/ACLK/CA2"/>
<pin name="P2_1/TAINCLK/CA3"/>
<pin name="P2_2/CAOUT/TA0/CA4"/>
<pin name="P2_3/CA0/TA1"/>
<pin name="P2_4/CA1/TA2"/>
<pin name="P2_5/ROSC/CA5"/>
<pin name="P2_6/ADC12CLK/CA6"/>
<pin name="P2_7/TA0/CA7"/>
<pin name="P3_0/UCB0STE/UCA0CLK"/>
<pin name="P3_1/UCB0SIMO/UCB0SDA"/>
<pin name="P3_2/UCB0SOMI/UCB0SCL"/>
<pin name="P3_3/UCB0CLK/UCA0STE"/>
<pin name="P3_4/UCA0TXD/UCA0SIMO"/>
<pin name="P3_5/UCA0RXD/UCA0SOMI"/>
<pin name="P3_6/UCA1TXD/UCA1SIMO"/>
<pin name="P3_7/UCA1RXD/UCA1SOMI"/>
<pin name="P4_0/TB0"/>
<pin name="P4_1/TB1"/>
<pin name="P4_2/TB2"/>
<pin name="P4_3/TB3"/>
<pin name="P4_4/TB4"/>
<pin name="P4_5/TB5"/>
<pin name="P4_6/TB6"/>
<pin name="P4_7/TBCLK"/>
<pin name="P5_0/UCB1STE/UCA1CLK"/>
<pin name="P5_1/UCB1SIMO/UCB1SDA"/>
<pin name="P5_2/UCB1SOMI/UCB1SCL"/>
<pin name="P5_3/UCB1CLK/UCA1STE"/>
<pin name="P5_4/MCLK"/>
<pin name="P5_5/SMCLK"/>
<pin name="P5_6/ACLK"/>
<pin name="P5_7/TBOUTH/SVSOUT"/>
<pin name="XT2OUT" direction="out"/>
<pin name="XT2IN" direction="in"/>
<pin name="TDO/TDI"/>
<pin name="TDI/TCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="!RST!/NMI" direction="in"/>
<pin name="P6_0/A0"/>
<pin name="P6_1/A1"/>
<pin name="P6_2/A2"/>
<pin name="AVSS" direction="pwr"/>
<pin name="DVSS" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="MSP430F24X1">
<pin name="DVCC" direction="pwr"/>
<pin name="P6_3"/>
<pin name="P6_4"/>
<pin name="P6_5"/>
<pin name="P6_6"/>
<pin name="P6_7/SVSIN"/>
<pin name="RESERVED" direction="out"/>
<pin name="XIN" direction="in"/>
<pin name="XOUT" direction="out"/>
<pin name="DVSS" direction="in"/>
<pin name="DVSS@1" direction="in"/>
<pin name="P1_0/TACLK/CAOUT"/>
<pin name="P1_1/TA0"/>
<pin name="P1_2/TA1"/>
<pin name="P1_3/TA2"/>
<pin name="P1_4/SMCLK"/>
<pin name="P1_5/TA0"/>
<pin name="P1_6/TA1"/>
<pin name="P1_7/TA2"/>
<pin name="P2_0/ACLK/CA2"/>
<pin name="P2_1/TAINCLK/CA3"/>
<pin name="P2_2/CAOUT/TA0/CA4"/>
<pin name="P2_3/CA0/TA1"/>
<pin name="P2_4/CA1/TA2"/>
<pin name="P2_5/ROSC/CA5"/>
<pin name="P2_6/ADC12CLK/CA6"/>
<pin name="P2_7/TA0/CA7"/>
<pin name="P3_0/UCB0STE/UCA0CLK"/>
<pin name="P3_1/UCB0SIMO/UCB0SDA"/>
<pin name="P3_2/UCB0SOMI/UCB0SCL"/>
<pin name="P3_3/UCB0CLK/UCA0STE"/>
<pin name="P3_4/UCA0TXD/UCA0SIMO"/>
<pin name="P3_5/UCA0RXD/UCA0SOMI"/>
<pin name="P3_6/UCA1TXD/UCA1SIMO"/>
<pin name="P3_7/UCA1RXD/UCA1SOMI"/>
<pin name="P4_0/TB0"/>
<pin name="P4_1/TB1"/>
<pin name="P4_2/TB2"/>
<pin name="P4_3/TB3"/>
<pin name="P4_4/TB4"/>
<pin name="P4_5/TB5"/>
<pin name="P4_6/TB6"/>
<pin name="P4_7/TBCLK"/>
<pin name="P5_0/UCB1STE/UCA1CLK"/>
<pin name="P5_1/UCB1SIMO/UCB1SDA"/>
<pin name="P5_2/UCB1SOMI/UCB1SCL"/>
<pin name="P5_3/UCB1CLK/UCA1STE"/>
<pin name="P5_4/MCLK"/>
<pin name="P5_5/SMCLK"/>
<pin name="P5_6/ACLK"/>
<pin name="P5_7/TBOUTH/SVSOUT"/>
<pin name="XT2OUT" direction="out"/>
<pin name="XT2IN" direction="in"/>
<pin name="TDO/TDI"/>
<pin name="TDI/TCLK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TCK" direction="in"/>
<pin name="!RST!/NMI" direction="in"/>
<pin name="P6_0"/>
<pin name="P6_1"/>
<pin name="P6_2"/>
<pin name="AVSS" direction="pwr"/>
<pin name="DVSS@2" direction="pwr"/>
<pin name="AVCC" direction="pwr"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="CC2531">
<pin name="AVDD@1" direction="pwr"/>
<pin name="AVDD@2" direction="pwr"/>
<pin name="AVDD@3" direction="pwr"/>
<pin name="AVDD@4" direction="pwr"/>
<pin name="AVDD@5" direction="pwr"/>
<pin name="AVDD@6" direction="pwr"/>
<pin name="DCOUPL" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DGND_USB" direction="pwr"/>
<pin name="USB_P"/>
<pin name="USB_N"/>
<pin name="DVDD_USB" direction="pwr"/>
<pin name="P0_0"/>
<pin name="P0_1"/>
<pin name="P0_2"/>
<pin name="P0_3"/>
<pin name="P0_4"/>
<pin name="P0_5"/>
<pin name="P0_6"/>
<pin name="P0_7"/>
<pin name="P1_0"/>
<pin name="P1_1"/>
<pin name="P1_2"/>
<pin name="P1_3"/>
<pin name="P1_4"/>
<pin name="P1_5"/>
<pin name="P1_6"/>
<pin name="P1_7"/>
<pin name="P2_0"/>
<pin name="P2_1"/>
<pin name="P2_2"/>
<pin name="P2_3/XOSC32K_Q2"/>
<pin name="P2_4/XOSC32K_Q1"/>
<pin name="RBIAS"/>
<pin name="RESET_N" direction="in"/>
<pin name="RF_N"/>
<pin name="RF_P"/>
<pin name="XOSC_Q1"/>
<pin name="XOSC_Q2"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="ISO1176">
<pin name="R" direction="in"/>
<pin name="!RE" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="GND1@1" direction="in"/>
<pin name="GND2@1" direction="in"/>
<pin name="VCC1" direction="in"/>
<pin name="VCC2" direction="in"/>
<pin name="DE" direction="in"/>
<pin name="D" direction="in"/>
<pin name="PV" direction="in"/>
<pin name="GND1@2" direction="in"/>
<pin name="GND2@2" direction="in"/>
<pin name="NC@1" direction="in"/>
<pin name="NC@2" direction="in"/>
<pin name="ISODE" direction="in"/>
</symbol>
<symbol name="DS1232LP">
<pin name="!PBRST" direction="in"/>
<pin name="TD" direction="in"/>
<pin name="TOL" direction="in"/>
<pin name="RST" direction="out"/>
<pin name="!RST" direction="out"/>
<pin name="!ST" direction="in"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="TPS5410">
<pin name="VIN" direction="in"/>
<pin name="ENA" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VSENSE" direction="in"/>
<pin name="BOOT" direction="out"/>
<pin name="PH" direction="out"/>
</symbol>
<symbol name="BQ78PL114">
<pin name="CHG" direction="out"/>
<pin name="DSG" direction="out"/>
<pin name="PRE" direction="out"/>
<pin name="EFCIC" direction="in"/>
<pin name="EFCID" direction="in"/>
<pin name="CCBAT" direction="in"/>
<pin name="CCPACK" direction="in"/>
<pin name="VLDO1" direction="pwr"/>
<pin name="CSBAT" direction="in"/>
<pin name="CSPACK" direction="in"/>
<pin name="OSCI" direction="in"/>
<pin name="OSCO" direction="out"/>
<pin name="SDO0" direction="out"/>
<pin name="SDI1" direction="in"/>
<pin name="P1N" direction="out"/>
<pin name="P2S" direction="out"/>
<pin name="P2N" direction="out"/>
<pin name="SDO2" direction="out"/>
<pin name="SDI3" direction="in"/>
<pin name="P3S" direction="out"/>
<pin name="P3N" direction="out"/>
<pin name="P4S" direction="out"/>
<pin name="P4N" direction="out"/>
<pin name="P-LAN"/>
<pin name="RSTN" direction="in"/>
<pin name="NC-IO"/>
<pin name="NC-I" direction="in"/>
<pin name="NC" direction="nc"/>
<pin name="NC@1" direction="nc"/>
<pin name="SPROT" direction="out"/>
<pin name="LEDEN"/>
<pin name="LED1" direction="out"/>
<pin name="LED2" direction="out"/>
<pin name="LED3" direction="out"/>
<pin name="LED4" direction="out"/>
<pin name="LED5" direction="out"/>
<pin name="SMBCLK"/>
<pin name="SMBDAT"/>
<pin name="V4" direction="in"/>
<pin name="XT4" direction="in"/>
<pin name="XT3" direction="in"/>
<pin name="V3" direction="in"/>
<pin name="VLDO2" direction="pwr"/>
<pin name="V2" direction="in"/>
<pin name="XT2" direction="in"/>
<pin name="XT1" direction="in"/>
<pin name="V1" direction="in"/>
<pin name="VSS" direction="in"/>
<pin name="EXP" direction="pas"/>
</symbol>
<symbol name="TMS320C5515">
<pin name="EM_BA[0]"/>
<pin name="DVDDEMIF" direction="pwr"/>
<pin name="EM_CS5"/>
<pin name="EM_CS1"/>
<pin name="DVDDEMIF@1" direction="pwr"/>
<pin name="EM_SDRAS"/>
<pin name="CLKOUT"/>
<pin name="CLKIN" direction="in"/>
<pin name="RTC_XO" direction="in"/>
<pin name="VDDA_ANA" direction="pwr"/>
<pin name="GPAIN1"/>
<pin name="ANA_LDOO" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="EM_BA[1]"/>
<pin name="EM_A[0]" direction="hiz"/>
<pin name="EM_CS0"/>
<pin name="EM_SDCAS"/>
<pin name="EM_DQM0"/>
<pin name="EM_R/W"/>
<pin name="SCL" direction="hiz"/>
<pin name="SDA" direction="hiz"/>
<pin name="RTC_XI" direction="in"/>
<pin name="VSSA_ANA" direction="pwr"/>
<pin name="GPAIN2"/>
<pin name="LDOI" direction="pwr"/>
<pin name="BG_CAP" direction="out"/>
<pin name="VSSA_ANA@1" direction="pwr"/>
<pin name="EM_A[4]" direction="hiz"/>
<pin name="EM_A[1]" direction="hiz"/>
<pin name="EM_CS4"/>
<pin name="EM_D[11]" direction="hiz"/>
<pin name="EM_CS2"/>
<pin name="INT0" direction="in"/>
<pin name="CLK_SEL" direction="in"/>
<pin name="CVDDRTC" direction="pwr"/>
<pin name="VSSRTC" direction="pwr"/>
<pin name="VDDA_PLL" direction="pwr"/>
<pin name="VDDA_PLL@1"/>
<pin name="RSV0" direction="in"/>
<pin name="RSV5" direction="in"/>
<pin name="RSV4" direction="in"/>
<pin name="EM_A[5]" direction="hiz"/>
<pin name="EM_A[3]" direction="hiz"/>
<pin name="EM_D[10]" direction="hiz"/>
<pin name="EM_D[3]" direction="hiz"/>
<pin name="EM_WAIT2" direction="in"/>
<pin name="RESET" direction="in"/>
<pin name="VSS@2"/>
<pin name="VSSA_PLL" direction="pwr"/>
<pin name="GPAIN0"/>
<pin name="VSSA_PLL@1" direction="pwr"/>
<pin name="DSP_LDO_EN" direction="in"/>
<pin name="VSS@3" direction="in"/>
<pin name="RSV3" direction="in"/>
<pin name="EM_A[2]" direction="hiz"/>
<pin name="EM_A[16]/GP[22]" direction="hiz"/>
<pin name="EM_D[8]" direction="hiz"/>
<pin name="EM_OE"/>
<pin name="EM_A[16]/GP[22]@1" direction="hiz"/>
<pin name="INT1" direction="in"/>
<pin name="WAKEUP" direction="hiz"/>
<pin name="DVDDEMIF@2" direction="pwr"/>
<pin name="DSP_LDOO" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="hiz"/>
<pin name="VSS@7" direction="hiz"/>
<pin name="VSS@8" direction="hiz"/>
<pin name="EM_D[9]" direction="hiz"/>
<pin name="EM_A[17]/GP[23]@1" direction="pwr"/>
<pin name="DVDDIO" direction="pwr"/>
<pin name="DVDDRTC" direction="pwr"/>
<pin name="DVDDEMIF@3" direction="pwr"/>
<pin name="USB_VSSOSC" direction="pwr"/>
<pin name="USB_LDOO" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="EM_WAIT4" direction="in"/>
<pin name="USB_VSSOSC@1" direction="hiz"/>
<pin name="EM_D[0]" direction="hiz"/>
<pin name="LDOI@1" direction="pwr"/>
<pin name="LDOI@2" direction="pwr"/>
<pin name="EM_A[18]/GP[24]@1" direction="pwr"/>
<pin name="USB_R1"/>
<pin name="USB_VSSREF" direction="pwr"/>
<pin name="EM_A[19]/GP[25]@1" direction="pwr"/>
<pin name="DVDDEMIF@4" direction="pwr"/>
<pin name="VSS@11" direction="in"/>
<pin name="VSS@12" direction="out"/>
<pin name="EM_WE"/>
<pin name="USB_VDDPLL@1" direction="hiz"/>
<pin name="EM_D[7]" direction="hiz"/>
<pin name="EM_WAIT5" direction="in"/>
<pin name="USB_VSSREF@1" direction="pwr"/>
<pin name="USB_VSSPLL@1" direction="pwr"/>
<pin name="CVDD" direction="pwr"/>
<pin name="USB_VDDOSC@1" direction="pwr"/>
<pin name="USB_VDDA1P3" direction="pwr"/>
<pin name="USB_VSSA3P3" direction="pwr"/>
<pin name="USB_VDDA3P3" direction="pwr"/>
<pin name="USB_VSS1P3" direction="pwr"/>
<pin name="USB_DP"/>
<pin name="EM_A[8]" direction="hiz"/>
<pin name="DVDDEMIF@5" direction="hiz"/>
<pin name="VSS@13" direction="hiz"/>
<pin name="DVDDEMIF@6" direction="hiz"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="USB_VSSA1P3@1" direction="pwr"/>
<pin name="USB_VDDA1P3@1" direction="pwr"/>
<pin name="RSV1" direction="pwr"/>
<pin name="USB_VSSA3P3@1" direction="pwr"/>
<pin name="USB_VBUS"/>
<pin name="USB_VDDA3P3@1" direction="pwr"/>
<pin name="USB_DM"/>
<pin name="USB_VSS1P3@1" direction="hiz"/>
<pin name="EM_A[11]/_ALE_" direction="hiz"/>
<pin name="EM_D[14]" direction="hiz"/>
<pin name="EM_D[13]" direction="hiz"/>
<pin name="EM_D[6]" direction="hiz"/>
<pin name="EM_A[20]/GP[26]@1" direction="in"/>
<pin name="DVDDEMIF@7" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="MMC1_D2/GP[10]" direction="hiz"/>
<pin name="EM_A[13]" direction="hiz"/>
<pin name="EM_A[10]" direction="hiz"/>
<pin name="USB_VDD1P3@1" direction="hiz"/>
<pin name="EM_D[4]" direction="hiz"/>
<pin name="EMU0" direction="hiz"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="MMC0_D0/I2S0_DX/GP[2]" direction="hiz"/>
<pin name="MMC0_CLK/I2S0_CLK/GP[0]" direction="hiz"/>
<pin name="DVDDIO@1" direction="hiz"/>
<pin name="VSS@17" direction="hiz"/>
<pin name="VSS@18" direction="hiz"/>
<pin name="CVDD@3" direction="hiz"/>
<pin name="VSS@19" direction="hiz"/>
<pin name="DVDDIO@2" direction="hiz"/>
<pin name="VSS@20"/>
<pin name="EM_CS3"/>
<pin name="MMC1_D2/GP[10]@1" direction="hiz"/>
<pin name="TCK" direction="in"/>
<pin name="TDO"/>
<pin name="XF"/>
<pin name="TRST" direction="in"/>
<pin name="CVDD@4" direction="hiz"/>
<pin name="MMC0_CMD/I2S0_FS/GP[1]" direction="hiz"/>
<pin name="MMC1_D1/I2S1_RX/GP[9]" direction="hiz"/>
<pin name="MMC1_CLK/I2S1_CLK/GP[6]" direction="hiz"/>
<pin name="MMC1_D0/2S1_DX/GP[8]" direction="hiz"/>
<pin name="MMC0_D0/I2S0_DX/GP[2]@1" direction="hiz"/>
<pin name="MMC0_D0/I2S0_DX/GP[2]@2"/>
<pin name="LCD_EN_RDB/"/>
<pin name="MMC0_CLK/I2S0_CLK/GP[0]@1" direction="hiz"/>
<pin name="MMC0_CLK/I2S0_CLK/GP[0]@2" direction="hiz"/>
<pin name="LCD_D[1]/SPI_TX" direction="hiz"/>
<pin name="MMC0_D3/GP[5]@1" direction="hiz"/>
<pin name="LCD_D[4]/GP[14]" direction="hiz"/>
<pin name="MMC0_D2/GP[4]@1" direction="hiz"/>
<pin name="LCD_D8]/I2S2_CLK/GP[18]/SPI_CLK" direction="hiz"/>
<pin name="MMC1_D3/GP[11]@1" direction="hiz"/>
<pin name="LCD_D[12]/UART_RTS/GP[28]/I2S3_CLK" direction="hiz"/>
<pin name="MMC1_CMD/I2S1_FS/GP[7]@1"/>
<pin name="MMC1_CMD/I2S1_FS/GP[7]@2" direction="pwr"/>
<pin name="EM_DQM1"/>
<pin name="LCD_CS0_E0/" direction="hiz"/>
<pin name="LCD_RW_WRB/" direction="hiz"/>
<pin name="LCD_D[0]/SPI_RX" direction="hiz"/>
<pin name="LCD_D[2]/GP[12]" direction="hiz"/>
<pin name="XF@1" direction="hiz"/>
<pin name="LCD_D[7]/GP[17]" direction="hiz"/>
<pin name="LCD_D[9]/I2S2_FS/GP[19]/SPI_CS0" direction="hiz"/>
<pin name="MMC0_D1/I2S0_RX/GP[3]@1" direction="hiz"/>
<pin name="MMC0_D1/I2S0_RX/GP[3]@2" direction="hiz"/>
<pin name="LCD_D[15]/UART_TXD/GP[31]/I2S3_DX" direction="hiz"/>
</symbol>
<symbol name="UC384D">
<pin name="RT/CT" direction="in"/>
<pin name="VFB" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="ISENSE" direction="in"/>
<pin name="REF" direction="out"/>
<pin name="VC" direction="pas"/>
<pin name="OUT" direction="out"/>
<pin name="PGND" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="UC384P">
<pin name="RT/CT" direction="in"/>
<pin name="VFB" direction="in"/>
<pin name="COMP" direction="pas"/>
<pin name="ISENSE" direction="in"/>
<pin name="REF" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="CC2540">
<pin name="DGND_USB" direction="pwr"/>
<pin name="USB_P"/>
<pin name="USB_N"/>
<pin name="DVDD_USB" direction="pwr"/>
<pin name="P1_5"/>
<pin name="P1_4"/>
<pin name="P1_3"/>
<pin name="P1_2"/>
<pin name="P1_1"/>
<pin name="DVDD2" direction="pwr"/>
<pin name="P1_0"/>
<pin name="P0_7"/>
<pin name="P0_6"/>
<pin name="P0_5"/>
<pin name="P0_4"/>
<pin name="P0_3"/>
<pin name="P0_2"/>
<pin name="P0_1"/>
<pin name="P0_0"/>
<pin name="RESET_N" direction="in"/>
<pin name="AVDD5" direction="pwr"/>
<pin name="XOSC_Q1"/>
<pin name="XOSC_Q2"/>
<pin name="AVDD3" direction="pwr"/>
<pin name="RF_P" direction="in"/>
<pin name="RF_N" direction="in"/>
<pin name="AVDD2" direction="pwr"/>
<pin name="AVDD1" direction="pwr"/>
<pin name="AVDD4" direction="pwr"/>
<pin name="RBIAS"/>
<pin name="AVDD6" direction="pwr"/>
<pin name="P2_4/XOSC32K_Q1"/>
<pin name="P2_3/XOSC32K_Q2"/>
<pin name="P2_2"/>
<pin name="P2_1"/>
<pin name="P2_0"/>
<pin name="P1_7"/>
<pin name="P1_6"/>
<pin name="DVDD1" direction="pwr"/>
<pin name="DCOUPL" direction="pwr"/>
</symbol>
<symbol name="ANTENNA">
<pin name="ANTENNA" direction="in"/>
</symbol>
<symbol name="TPS62120">
<pin name="VIN" direction="in"/>
<pin name="EN" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="PG" direction="pas"/>
<pin name="SGND" direction="pas"/>
<pin name="VOUT" direction="out"/>
<pin name="FB" direction="in"/>
<pin name="SW" direction="out"/>
</symbol>
<symbol name="BQ24022">
<pin name="AC" direction="in"/>
<pin name="USB"/>
<pin name="STAT1"/>
<pin name="STAT2"/>
<pin name="VSS" direction="pwr"/>
<pin name="ISET1" direction="in"/>
<pin name="ISET2" direction="in"/>
<pin name="1CE" direction="in"/>
<pin name="TS" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="TLC450X">
<pin name="+" direction="in"/>
<pin name="-" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="TLC450P">
<description>OP-AMP power pins</description>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="TPS63060">
<pin name="EN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="L1" direction="in"/>
<pin name="L2" direction="in"/>
<pin name="PS/SYNC" direction="in"/>
<pin name="PG" direction="out"/>
<pin name="PGND" direction="pwr"/>
<pin name="VIN" direction="in"/>
<pin name="VOUT" direction="out"/>
<pin name="VAUX" direction="pwr"/>
</symbol>
<symbol name="LM3401">
<pin name="VIN" direction="in"/>
<pin name="DIM" direction="pas"/>
<pin name="HYS" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="SNS" direction="in"/>
<pin name="CS" direction="in"/>
<pin name="HG" direction="out"/>
<pin name="ILIM" direction="in"/>
</symbol>
<symbol name="DM385_AAR">
<pin name="DDR0A13"/>
<pin name="DDR0A14"/>
<pin name="DDR0A1"/>
<pin name="DDR0A15"/>
<pin name="DDR0CS0N"/>
<pin name="RSV42"/>
<pin name="DDR0ODT0"/>
<pin name="DDR0RST"/>
<pin name="DDR0CKE"/>
<pin name="DDR0RASN"/>
<pin name="DDR0CASN"/>
<pin name="DDR0A11"/>
<pin name="DDR0A0"/>
<pin name="DDR0A10"/>
<pin name="DDR0BA1"/>
<pin name="DDR0A7"/>
<pin name="DDR0A12"/>
<pin name="DDR0A2"/>
<pin name="DDR0A6"/>
<pin name="DDR0A9"/>
<pin name="DDR0A8"/>
<pin name="DDR0A4"/>
<pin name="DDR0A3"/>
<pin name="DDR0CLK"/>
<pin name="DDR0CLKN"/>
<pin name="DDR0A5"/>
<pin name="DDR0BA0"/>
<pin name="DDR0WEN"/>
<pin name="DDR0BA2"/>
<pin name="DDR0DQM3"/>
<pin name="DDR0DQM2"/>
<pin name="DDR0DQM1"/>
<pin name="DDR0DQM0"/>
<pin name="DDR0DQS3"/>
<pin name="DDR0DQS2"/>
<pin name="DDR0DQS1"/>
<pin name="DDR0DQS0"/>
<pin name="DDR0D31"/>
<pin name="DDR0D30"/>
<pin name="DDR0D29"/>
<pin name="DDR0D28"/>
<pin name="DDR0D27"/>
<pin name="DDR0D26"/>
<pin name="DDR0D25"/>
<pin name="DDR0D24"/>
<pin name="DDR0D23"/>
<pin name="DDR0D22"/>
<pin name="DDR0D21"/>
<pin name="DDR0D20"/>
<pin name="DDR0D19"/>
<pin name="DDR0D18"/>
<pin name="DDR0D17"/>
<pin name="DDR0D16"/>
<pin name="DDR0D15"/>
<pin name="DDR0D14"/>
<pin name="DDR0D13"/>
<pin name="DDR0D12"/>
<pin name="DDR0D11"/>
<pin name="DDR0D10"/>
<pin name="DDR0D9"/>
<pin name="DDR0D8"/>
<pin name="DDR0D7"/>
<pin name="DDR0D6"/>
<pin name="DDR0D5"/>
<pin name="DDR0D4"/>
<pin name="DDR0D3"/>
<pin name="DDR0D2"/>
<pin name="DDR0D1"/>
<pin name="DDR0D0"/>
<pin name="EMAC0MTXEN_EMAC1RGRXD2"/>
<pin name="EMAC0MTXD7_EMAC1RGTXD3"/>
<pin name="EMAC0MTXD6_EMAC1RGRXD0"/>
<pin name="EMAC0MTXD5_EMAC1RGTXC"/>
<pin name="EMAC0MTXD4_EMAC1RGTXD2"/>
<pin name="EMAC0MTXD3_EMAC1RGTXD0"/>
<pin name="EMAC0MTXD2_EMAC1RGTXCTL"/>
<pin name="EMAC0MTXD1_EMAC1RGTXD1"/>
<pin name="EMAC0MTXD0_EMAC1RGRXD3"/>
<pin name="EMAC0GMTCLK_EMAC1RGRXC"/>
<pin name="EMAC0MRXDV_EMAC1RGRXD1"/>
<pin name="EMAC0MRXD7_EMAC0RGTXD1"/>
<pin name="EMAC0MRXD6_EMAC0RGTXD2"/>
<pin name="EMAC0MRXD5_EMAC0RGTXD3"/>
<pin name="EMAC0MRXD4_EMAC0RGRXD3"/>
<pin name="EMAC0MRXD3_EMAC1RGRXCTL"/>
<pin name="EMAC0MRXD2_EMAC0RGRXD1"/>
<pin name="EMAC0MRXD1_EMAC0RGRXD0"/>
<pin name="EMAC0MRCLK_EMAC0RGTXC"/>
<pin name="EMAC0MRXER_EMAC0RGTXCTL"/>
<pin name="EMAC0MRXD0_EMAC0RGTXD0"/>
<pin name="EMAC0MCRS_EMAC0RGRXD2"/>
<pin name="EMAC0MCOL_EMAC0RGRXCTL"/>
<pin name="EMAC0MTCLK_EMAC0RGRXC"/>
<pin name="MDIO"/>
<pin name="MDCLK"/>
<pin name="EMACRMREFCLK"/>
<pin name="GPMCCS3N"/>
<pin name="GPMCCS4N"/>
<pin name="SD2DAT7"/>
<pin name="SD2DAT6"/>
<pin name="SD2DAT5"/>
<pin name="SD2DAT4"/>
<pin name="SD2DAT3"/>
<pin name="SD2DAT2SDRWN"/>
<pin name="SD2SCLK"/>
<pin name="SD2DAT1SDIRQN"/>
<pin name="SD2DAT0"/>
<pin name="GPMCCS0N"/>
<pin name="GPMCCS1N"/>
<pin name="GPMCCS2N"/>
<pin name="GPMCCLK"/>
<pin name="GPMCADVNALE"/>
<pin name="GPMCOEREN"/>
<pin name="GPMCWEN"/>
<pin name="GPMCBE0NCLE"/>
<pin name="GPMCBE1N"/>
<pin name="GPMCWAIT0"/>
<pin name="GPMCD0"/>
<pin name="GPMCD1"/>
<pin name="GPMCD2"/>
<pin name="GPMCD3"/>
<pin name="GPMCD4"/>
<pin name="GPMCD5"/>
<pin name="GPMCD6"/>
<pin name="GPMCD7"/>
<pin name="GPMCD8"/>
<pin name="GPMCD9"/>
<pin name="GPMCD10"/>
<pin name="GPMCD11"/>
<pin name="GPMCD12"/>
<pin name="GPMCD13"/>
<pin name="GPMCD14"/>
<pin name="GPMCD15"/>
<pin name="GPMCA23"/>
<pin name="GPMCA22"/>
<pin name="GPMCA21"/>
<pin name="GPMCA20"/>
<pin name="GPMCA19"/>
<pin name="GPMCA18"/>
<pin name="GPMCA17"/>
<pin name="GPMCA16"/>
<pin name="VOUT1BCBC2"/>
<pin name="VOUT1RCR2"/>
<pin name="VOUT1RCR3"/>
<pin name="VOUT1GYYC2"/>
<pin name="VOUT1RCR9"/>
<pin name="VOUT1RCR8"/>
<pin name="VOUT1RCR7"/>
<pin name="VOUT1RCR6"/>
<pin name="VOUT1RCR5"/>
<pin name="VOUT1RCR4"/>
<pin name="VOUT1GYYC9"/>
<pin name="VOUT1GYYC8"/>
<pin name="VOUT1GYYC7"/>
<pin name="VOUT1GYYC6"/>
<pin name="VOUT1GYYC5"/>
<pin name="VOUT1GYYC4"/>
<pin name="VOUT1GYYC3"/>
<pin name="VOUT1BCBC9"/>
<pin name="VOUT1BCBC8"/>
<pin name="VOUT1BCBC7"/>
<pin name="VOUT1BCBC6"/>
<pin name="VOUT1BCBC5"/>
<pin name="VOUT1BCBC4"/>
<pin name="VOUT1BCBC3"/>
<pin name="VOUT1AVID"/>
<pin name="VOUT1VSYNC"/>
<pin name="VOUT1HSYNC"/>
<pin name="VOUT1CLK"/>
<pin name="I2C1SCL"/>
<pin name="I2C1SDA"/>
<pin name="VOUT1FLD"/>
<pin name="VOUT1BCBC0"/>
<pin name="VOUT1BCBC1"/>
<pin name="VOUT1RCR0"/>
<pin name="VOUT1RCR1"/>
<pin name="VOUT1GYYC0"/>
<pin name="VOUT1GYYC1"/>
<pin name="VOUT0FLD"/>
<pin name="VIN0BFLD"/>
<pin name="VIN0AFLD1"/>
<pin name="VIN0BDE"/>
<pin name="VIN0ADE1"/>
<pin name="VIN0AD23"/>
<pin name="VIN0AD22"/>
<pin name="VIN0AD21"/>
<pin name="VIN0AD20"/>
<pin name="VIN0AD19"/>
<pin name="VIN0AD18"/>
<pin name="VIN0AD17"/>
<pin name="VIN0AD16"/>
<pin name="VIN0BCLK"/>
<pin name="VIN0ADE"/>
<pin name="VIN0AFLD"/>
<pin name="VIN0ACLK"/>
<pin name="VIN0AHSYNC"/>
<pin name="HDDACVSYNC"/>
<pin name="HDDACHSYNC"/>
<pin name="VIN0AVSYNC"/>
<pin name="VIN0AD15BD7"/>
<pin name="VIN0AD14BD6"/>
<pin name="VIN0AD13BD5"/>
<pin name="VIN0AD12BD4"/>
<pin name="VIN0AD11BD3"/>
<pin name="VIN0AD10BD2"/>
<pin name="VIN0AD9BD1"/>
<pin name="VIN0AD8BD0"/>
<pin name="VIN0AD7"/>
<pin name="VIN0AD6"/>
<pin name="VIN0AD5"/>
<pin name="VIN0AD4"/>
<pin name="VIN0AD3"/>
<pin name="VIN0AD2"/>
<pin name="VIN0AD1"/>
<pin name="VIN0AD0"/>
<pin name="EMU1"/>
<pin name="EMU0"/>
<pin name="VOUT0CLK"/>
<pin name="VOUT0HSYNC"/>
<pin name="VOUT0VSYNC"/>
<pin name="VOUT0AVID"/>
<pin name="VOUT0BCBC2"/>
<pin name="VOUT0BCBC3"/>
<pin name="VOUT0BCBC4"/>
<pin name="VOUT0BCBC5"/>
<pin name="VOUT0BCBC6"/>
<pin name="VOUT0BCBC7"/>
<pin name="VOUT0BCBC8"/>
<pin name="VOUT0BCBC9"/>
<pin name="VOUT0GYYC2"/>
<pin name="VOUT0GYYC3"/>
<pin name="VOUT0GYYC4"/>
<pin name="VOUT0GYYC5"/>
<pin name="VOUT0GYYC6"/>
<pin name="VOUT0GYYC7"/>
<pin name="VOUT0GYYC8"/>
<pin name="VOUT0GYYC9"/>
<pin name="VOUT0RCR2"/>
<pin name="VOUT0RCR3"/>
<pin name="VOUT0RCR4"/>
<pin name="VOUT0RCR5"/>
<pin name="VOUT0RCR6"/>
<pin name="VOUT0RCR7"/>
<pin name="VOUT0RCR8"/>
<pin name="VOUT0RCR9"/>
<pin name="USB0DRVVBUS"/>
<pin name="UART2TXD"/>
<pin name="UART0RXD"/>
<pin name="UART0TXD"/>
<pin name="UART0CTSN"/>
<pin name="UART0RTSN"/>
<pin name="UART0DCDN"/>
<pin name="UART0DSRN"/>
<pin name="UART0DTRN"/>
<pin name="UART0RIN"/>
<pin name="SPI0SCS1N"/>
<pin name="UART2RXD"/>
<pin name="SPI0SCS0N"/>
<pin name="SPI0SCLK"/>
<pin name="SPI0D1"/>
<pin name="SPI0D0"/>
<pin name="SPI1SCS0N"/>
<pin name="SPI1SCLK"/>
<pin name="SPI1D1"/>
<pin name="SPI1D0"/>
<pin name="I2C0SCL"/>
<pin name="I2C0SDA"/>
<pin name="DEVOSCWAKE"/>
<pin name="SD1CLK"/>
<pin name="SD1CMD"/>
<pin name="SD1DAT0"/>
<pin name="SD1DAT1SDIRQN"/>
<pin name="SD1DAT2SDRWN"/>
<pin name="SD1DAT3"/>
<pin name="SD0DAT3"/>
<pin name="SD0DAT2SDRWN"/>
<pin name="SD0DAT1SDIRQN"/>
<pin name="SD0DAT0"/>
<pin name="SD0CMD"/>
<pin name="SD0CLK"/>
<pin name="SD0DAT6"/>
<pin name="SD0DAT7"/>
<pin name="MCA1AXR1"/>
<pin name="MCA1AXR0"/>
<pin name="MCA1AFSX"/>
<pin name="MCA1ACLKX"/>
<pin name="MCA1AFSR"/>
<pin name="MCA1ACLKR"/>
<pin name="MCA0AXR3"/>
<pin name="MCA0AXR4"/>
<pin name="MCA0AXR5"/>
<pin name="MCA0ACLKX"/>
<pin name="MCA0AFSX"/>
<pin name="MCA0ACLKR"/>
<pin name="MCA0AXR2"/>
<pin name="MCA0AXR1"/>
<pin name="MCA0AXR0"/>
<pin name="MCA0AFSR"/>
<pin name="AUDCLKIN0"/>
<pin name="AUDCLKIN1"/>
<pin name="AUDCLKIN2"/>
<pin name="RESETN"/>
<pin name="NMIN"/>
<pin name="RSTOUTWDOUTN"/>
<pin name="CLKIN32"/>
<pin name="PORN" direction="in"/>
<pin name="TRSTN" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DDR0DQS0N"/>
<pin name="DDR0DQS1N"/>
<pin name="DDR0DQS2N"/>
<pin name="DDR0DQS3N"/>
<pin name="VREFSSTLDDR0" direction="pas"/>
<pin name="VSSADEVOSC" direction="pwr"/>
<pin name="VSSAAUXOSC" direction="pwr"/>
<pin name="VSSAVDAC" direction="pwr"/>
<pin name="VSSACSI2@1" direction="pwr"/>
<pin name="VSSACSI2@2" direction="pwr"/>
<pin name="VSSAHDMI@1" direction="pwr"/>
<pin name="VSSAHDMI@2" direction="pwr"/>
<pin name="VSSAUSB@1" direction="pwr"/>
<pin name="VSSAUSB@2" direction="pwr"/>
<pin name="VSSAUSB@3" direction="pwr"/>
<pin name="RSV4" direction="pas"/>
<pin name="RSV5" direction="pas"/>
<pin name="CVDDARM@1" direction="pwr"/>
<pin name="CVDDARM@2" direction="pwr"/>
<pin name="CVDDARM@3" direction="pwr"/>
<pin name="CVDDARM@4" direction="pwr"/>
<pin name="CVDDARM@5" direction="pwr"/>
<pin name="CVDDARM@6" direction="pwr"/>
<pin name="CVDDHDVICP@1" direction="pwr"/>
<pin name="CVDDHDVICP@2" direction="pwr"/>
<pin name="CVDDHDVICP@3" direction="pwr"/>
<pin name="CVDDHDVICP@4" direction="pwr"/>
<pin name="CVDDHDVICP@5" direction="pwr"/>
<pin name="LDOCAPSERDESCLK" direction="pas"/>
<pin name="VDDAARMPLL1P8" direction="pwr"/>
<pin name="LDOCAPARM" direction="pas"/>
<pin name="LDOCAPHDVICP" direction="pas"/>
<pin name="VDDAAUDIOPLL1P8" direction="pwr"/>
<pin name="VDDAVDAC1P8" direction="pwr"/>
<pin name="VDDACSI21P8" direction="pwr"/>
<pin name="VDDADDRPLL1P8" direction="pwr"/>
<pin name="VDDAHDDAC1P1" direction="pwr"/>
<pin name="VDDAHDDAC1P8" direction="pwr"/>
<pin name="VDDAHDMI1P8" direction="pwr"/>
<pin name="VDDAL3L41P8" direction="pwr"/>
<pin name="VDDAHDVICPPLL1P8" direction="pwr"/>
<pin name="VDDAHDDACREF1P8" direction="pwr"/>
<pin name="VDDAVIDPLL1P8" direction="pwr"/>
<pin name="VDDAUSB01P8" direction="pwr"/>
<pin name="VDDAUSB11P8" direction="pwr"/>
<pin name="VDDAUSB3P3@1" direction="pwr"/>
<pin name="VDDAUSB3P3@2" direction="pwr"/>
<pin name="VDDAPCIE1P8" direction="pwr"/>
<pin name="RSV55" direction="pas"/>
<pin name="RSV54" direction="pas"/>
<pin name="LDOCAPARMRAM" direction="pas"/>
<pin name="LDOCAPRAM0" direction="pas"/>
<pin name="LDOCAPRAM1" direction="pas"/>
<pin name="LDOCAPRAM2" direction="pas"/>
<pin name="LDOCAPHDVICPRAM" direction="pas"/>
<pin name="VDDSOSC01P8" direction="pwr"/>
<pin name="VDDSOSC11P8" direction="pwr"/>
<pin name="VDDA1P8@1" direction="pwr"/>
<pin name="VDDA1P8@2" direction="pwr"/>
<pin name="VDDA1P8@3" direction="pwr"/>
<pin name="VDDA1P8@4" direction="pwr"/>
<pin name="VDDA1P8@5" direction="pwr"/>
<pin name="VDDA1P8@6" direction="pwr"/>
<pin name="VDDA1P8@7" direction="pwr"/>
<pin name="DVDDDDR0@1" direction="pwr"/>
<pin name="DVDDDDR0@2" direction="pwr"/>
<pin name="DVDDDDR0@3" direction="pwr"/>
<pin name="DVDDDDR0@4" direction="pwr"/>
<pin name="DVDDDDR0@5" direction="pwr"/>
<pin name="DVDDDDR0@6" direction="pwr"/>
<pin name="DVDDDDR0@7" direction="pwr"/>
<pin name="DVDDDDR0@8" direction="pwr"/>
<pin name="DVDDDDR0@9" direction="pwr"/>
<pin name="DVDDDDR0@10" direction="pwr"/>
<pin name="DVDDDDR0@11" direction="pwr"/>
<pin name="DVDDDDR0@12" direction="pwr"/>
<pin name="DVDDRGMII@1" direction="pwr"/>
<pin name="DVDDRGMII@2" direction="pwr"/>
<pin name="DVDDRGMII@3" direction="pwr"/>
<pin name="DVDDRGMII@4" direction="pwr"/>
<pin name="DVDDRGMII@5" direction="pwr"/>
<pin name="DVDDGPMC@1" direction="pwr"/>
<pin name="DVDDGPMC@2" direction="pwr"/>
<pin name="DVDDGPMC@3" direction="pwr"/>
<pin name="DVDDGPMC@4" direction="pwr"/>
<pin name="DVDDGPMC@5" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="DVDD@7" direction="pwr"/>
<pin name="DVDD@8" direction="pwr"/>
<pin name="DVDD@9" direction="pwr"/>
<pin name="DVDD@10" direction="pwr"/>
<pin name="DVDD@11" direction="pwr"/>
<pin name="DVDD@12" direction="pwr"/>
<pin name="DVDDC@1" direction="pwr"/>
<pin name="DVDDC@2" direction="pwr"/>
<pin name="DVDDC@3" direction="pwr"/>
<pin name="DVDDC@4" direction="pwr"/>
<pin name="DVDDC@5" direction="pwr"/>
<pin name="DVDDSD@1" direction="pwr"/>
<pin name="DVDDSD@2" direction="pwr"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="CVDD@7" direction="pwr"/>
<pin name="CVDD@8" direction="pwr"/>
<pin name="CVDD@9" direction="pwr"/>
<pin name="CVDD@10" direction="pwr"/>
<pin name="CVDD@11" direction="pwr"/>
<pin name="CVDD@12" direction="pwr"/>
<pin name="CVDD@13" direction="pwr"/>
<pin name="CVDD@14" direction="pwr"/>
<pin name="CVDD@15" direction="pwr"/>
<pin name="CVDD@16" direction="pwr"/>
<pin name="CVDD@17" direction="pwr"/>
<pin name="CVDD@18" direction="pwr"/>
<pin name="CVDD@19" direction="pwr"/>
<pin name="CVDD@20" direction="pwr"/>
<pin name="CVDD@21" direction="pwr"/>
<pin name="CVDD@22" direction="pwr"/>
<pin name="CVDD@23" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
<pin name="VSS@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="VSS@45" direction="pwr"/>
<pin name="VSS@46" direction="pwr"/>
<pin name="VSS@47" direction="pwr"/>
<pin name="VSS@48" direction="pwr"/>
<pin name="VSS@49" direction="pwr"/>
<pin name="VSS@50" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VSS@52" direction="pwr"/>
<pin name="VSS@53" direction="pwr"/>
<pin name="VSS@54" direction="pwr"/>
<pin name="VSS@55" direction="pwr"/>
<pin name="VSS@56" direction="pwr"/>
<pin name="VSS@57" direction="pwr"/>
<pin name="VSS@58" direction="pwr"/>
<pin name="VSS@59" direction="pwr"/>
<pin name="VSS@60" direction="pwr"/>
<pin name="VSS@61" direction="pwr"/>
<pin name="VSS@62" direction="pwr"/>
<pin name="VSS@63" direction="pwr"/>
<pin name="VSS@64" direction="pwr"/>
<pin name="VSS@65" direction="pwr"/>
<pin name="VSS@66" direction="pwr"/>
<pin name="VSS@67" direction="pwr"/>
<pin name="VSS@68" direction="pwr"/>
<pin name="VSS@69" direction="pwr"/>
<pin name="VSS@70" direction="pwr"/>
<pin name="VSS@71" direction="pwr"/>
<pin name="VSS@72" direction="pwr"/>
<pin name="VSS@73" direction="pwr"/>
<pin name="VSS@74" direction="pwr"/>
<pin name="VSS@75" direction="pwr"/>
<pin name="VSS@76" direction="pwr"/>
<pin name="VSS@77" direction="pwr"/>
<pin name="VSS@78" direction="pwr"/>
<pin name="VSS@79" direction="pwr"/>
<pin name="VSS@80" direction="pwr"/>
<pin name="VSS@81" direction="pwr"/>
<pin name="VSS@82" direction="pwr"/>
<pin name="VSS@83" direction="pwr"/>
<pin name="VSS@84" direction="pwr"/>
<pin name="VSS@85" direction="pwr"/>
<pin name="VSS@86" direction="pwr"/>
<pin name="VSS@87" direction="pwr"/>
<pin name="VSS@88" direction="pwr"/>
<pin name="VSS@89" direction="pwr"/>
<pin name="VSS@90" direction="pwr"/>
<pin name="VSS@91" direction="pwr"/>
<pin name="VSS@92" direction="pwr"/>
<pin name="VSS@93" direction="pwr"/>
<pin name="VSS@94" direction="pwr"/>
<pin name="VSS@95" direction="pwr"/>
<pin name="VSS@96" direction="pwr"/>
<pin name="VSS@97" direction="pwr"/>
<pin name="VSS@98" direction="pwr"/>
<pin name="VSS@99" direction="pwr"/>
<pin name="VSS@100" direction="pwr"/>
<pin name="VSS@101" direction="pwr"/>
<pin name="VSS@102" direction="pwr"/>
<pin name="VSS@103" direction="pwr"/>
<pin name="VSS@104" direction="pwr"/>
<pin name="VSS@105" direction="pwr"/>
</symbol>
<symbol name="DM385">
<pin name="DDR0A13"/>
<pin name="DDR0A14"/>
<pin name="DDR0A1"/>
<pin name="DDR0A15"/>
<pin name="DDR0CS0N"/>
<pin name="RSV42"/>
<pin name="DDR0ODT0"/>
<pin name="DDR0RST"/>
<pin name="DDR0CKE"/>
<pin name="DDR0RASN"/>
<pin name="DDR0CASN"/>
<pin name="DDR0A11"/>
<pin name="DDR0A0"/>
<pin name="DDR0A10"/>
<pin name="DDR0BA1"/>
<pin name="DDR0A7"/>
<pin name="DDR0A12"/>
<pin name="DDR0A2"/>
<pin name="DDR0A6"/>
<pin name="DDR0A9"/>
<pin name="DDR0A8"/>
<pin name="DDR0A4"/>
<pin name="DDR0A3"/>
<pin name="DDR0CLK"/>
<pin name="DDR0CLKN"/>
<pin name="DDR0A5"/>
<pin name="DDR0BA0"/>
<pin name="DDR0WEN"/>
<pin name="DDR0BA2"/>
<pin name="DDR0DQM3"/>
<pin name="DDR0DQM2"/>
<pin name="DDR0DQM1"/>
<pin name="DDR0DQM0"/>
<pin name="DDR0DQS3"/>
<pin name="DDR0DQS2"/>
<pin name="DDR0DQS1"/>
<pin name="DDR0DQS0"/>
<pin name="DDR0D31"/>
<pin name="DDR0D30"/>
<pin name="DDR0D29"/>
<pin name="DDR0D28"/>
<pin name="DDR0D27"/>
<pin name="DDR0D26"/>
<pin name="DDR0D25"/>
<pin name="DDR0D24"/>
<pin name="DDR0D23"/>
<pin name="DDR0D22"/>
<pin name="DDR0D21"/>
<pin name="DDR0D20"/>
<pin name="DDR0D19"/>
<pin name="DDR0D18"/>
<pin name="DDR0D17"/>
<pin name="DDR0D16"/>
<pin name="DDR0D15"/>
<pin name="DDR0D14"/>
<pin name="DDR0D13"/>
<pin name="DDR0D12"/>
<pin name="DDR0D11"/>
<pin name="DDR0D10"/>
<pin name="DDR0D9"/>
<pin name="DDR0D8"/>
<pin name="DDR0D7"/>
<pin name="DDR0D6"/>
<pin name="DDR0D5"/>
<pin name="DDR0D4"/>
<pin name="DDR0D3"/>
<pin name="DDR0D2"/>
<pin name="DDR0D1"/>
<pin name="DDR0D0"/>
<pin name="EMAC0MTXEN_EMAC1RGRXD2"/>
<pin name="EMAC0MTXD7_EMAC1RGTXD3"/>
<pin name="EMAC0MTXD6_EMAC1RGRXD0"/>
<pin name="EMAC0MTXD5_EMAC1RGTXC"/>
<pin name="EMAC0MTXD4_EMAC1RGTXD2"/>
<pin name="EMAC0MTXD3_EMAC1RGTXD0"/>
<pin name="EMAC0MTXD2_EMAC1RGTXCTL"/>
<pin name="EMAC0MTXD1_EMAC1RGTXD1"/>
<pin name="EMAC0MTXD0_EMAC1RGRXD3"/>
<pin name="EMAC0GMTCLK_EMAC1RGRXC"/>
<pin name="EMAC0MRXDV_EMAC1RGRXD1"/>
<pin name="EMAC0MRXD7_EMAC0RGTXD1"/>
<pin name="EMAC0MRXD6_EMAC0RGTXD2"/>
<pin name="EMAC0MRXD5_EMAC0RGTXD3"/>
<pin name="EMAC0MRXD4_EMAC0RGRXD3"/>
<pin name="EMAC0MRXD3_EMAC1RGRXCTL"/>
<pin name="EMAC0MRXD2_EMAC0RGRXD1"/>
<pin name="EMAC0MRXD1_EMAC0RGRXD0"/>
<pin name="EMAC0MRCLK_EMAC0RGTXC"/>
<pin name="EMAC0MRXER_EMAC0RGTXCTL"/>
<pin name="EMAC0MRXD0_EMAC0RGTXD0"/>
<pin name="EMAC0MCRS_EMAC0RGRXD2"/>
<pin name="EMAC0MCOL_EMAC0RGRXCTL"/>
<pin name="EMAC0MTCLK_EMAC0RGRXC"/>
<pin name="MDIO"/>
<pin name="MDCLK"/>
<pin name="EMACRMREFCLK"/>
<pin name="GPMCCS3N"/>
<pin name="GPMCCS4N"/>
<pin name="SD2DAT7"/>
<pin name="SD2DAT6"/>
<pin name="SD2DAT5"/>
<pin name="SD2DAT4"/>
<pin name="SD2DAT3"/>
<pin name="SD2DAT2SDRWN"/>
<pin name="SD2SCLK"/>
<pin name="SD2DAT1SDIRQN"/>
<pin name="SD2DAT0"/>
<pin name="GPMCCS0N"/>
<pin name="GPMCCS1N"/>
<pin name="GPMCCS2N"/>
<pin name="GPMCCLK"/>
<pin name="GPMCADVNALE"/>
<pin name="GPMCOEREN"/>
<pin name="GPMCWEN"/>
<pin name="GPMCBE0NCLE"/>
<pin name="GPMCBE1N"/>
<pin name="GPMCWAIT0"/>
<pin name="GPMCD0"/>
<pin name="GPMCD1"/>
<pin name="GPMCD2"/>
<pin name="GPMCD3"/>
<pin name="GPMCD4"/>
<pin name="GPMCD5"/>
<pin name="GPMCD6"/>
<pin name="GPMCD7"/>
<pin name="GPMCD8"/>
<pin name="GPMCD9"/>
<pin name="GPMCD10"/>
<pin name="GPMCD11"/>
<pin name="GPMCD12"/>
<pin name="GPMCD13"/>
<pin name="GPMCD14"/>
<pin name="GPMCD15"/>
<pin name="GPMCA23"/>
<pin name="GPMCA22"/>
<pin name="GPMCA21"/>
<pin name="GPMCA20"/>
<pin name="GPMCA19"/>
<pin name="GPMCA18"/>
<pin name="GPMCA17"/>
<pin name="GPMCA16"/>
<pin name="VOUT1BCBC2"/>
<pin name="VOUT1RCR2"/>
<pin name="VOUT1RCR3"/>
<pin name="VOUT1GYYC2"/>
<pin name="VOUT1RCR9"/>
<pin name="VOUT1RCR8"/>
<pin name="VOUT1RCR7"/>
<pin name="VOUT1RCR6"/>
<pin name="VOUT1RCR5"/>
<pin name="VOUT1RCR4"/>
<pin name="VOUT1GYYC9"/>
<pin name="VOUT1GYYC8"/>
<pin name="VOUT1GYYC7"/>
<pin name="VOUT1GYYC6"/>
<pin name="VOUT1GYYC5"/>
<pin name="VOUT1GYYC4"/>
<pin name="VOUT1GYYC3"/>
<pin name="VOUT1BCBC9"/>
<pin name="VOUT1BCBC8"/>
<pin name="VOUT1BCBC7"/>
<pin name="VOUT1BCBC6"/>
<pin name="VOUT1BCBC5"/>
<pin name="VOUT1BCBC4"/>
<pin name="VOUT1BCBC3"/>
<pin name="VOUT1AVID"/>
<pin name="VOUT1VSYNC"/>
<pin name="VOUT1HSYNC"/>
<pin name="VOUT1CLK"/>
<pin name="I2C1SCL"/>
<pin name="I2C1SDA"/>
<pin name="VOUT1FLD"/>
<pin name="VOUT1BCBC0"/>
<pin name="VOUT1BCBC1"/>
<pin name="VOUT1RCR0"/>
<pin name="VOUT1RCR1"/>
<pin name="VOUT1GYYC0"/>
<pin name="VOUT1GYYC1"/>
<pin name="VOUT0FLD"/>
<pin name="VIN0BFLD"/>
<pin name="VIN0AFLD1"/>
<pin name="VIN0BDE"/>
<pin name="VIN0ADE1"/>
<pin name="VIN0AD23"/>
<pin name="VIN0AD22"/>
<pin name="VIN0AD21"/>
<pin name="VIN0AD20"/>
<pin name="VIN0AD19"/>
<pin name="VIN0AD18"/>
<pin name="VIN0AD17"/>
<pin name="VIN0AD16"/>
<pin name="VIN0BCLK"/>
<pin name="VIN0ADE"/>
<pin name="VIN0AFLD"/>
<pin name="VIN0ACLK"/>
<pin name="VIN0AHSYNC"/>
<pin name="HDDACVSYNC"/>
<pin name="HDDACHSYNC"/>
<pin name="VIN0AVSYNC"/>
<pin name="VIN0AD15BD7"/>
<pin name="VIN0AD14BD6"/>
<pin name="VIN0AD13BD5"/>
<pin name="VIN0AD12BD4"/>
<pin name="VIN0AD11BD3"/>
<pin name="VIN0AD10BD2"/>
<pin name="VIN0AD9BD1"/>
<pin name="VIN0AD8BD0"/>
<pin name="VIN0AD7"/>
<pin name="VIN0AD6"/>
<pin name="VIN0AD5"/>
<pin name="VIN0AD4"/>
<pin name="VIN0AD3"/>
<pin name="VIN0AD2"/>
<pin name="VIN0AD1"/>
<pin name="VIN0AD0"/>
<pin name="EMU1"/>
<pin name="EMU0"/>
<pin name="VOUT0CLK"/>
<pin name="VOUT0HSYNC"/>
<pin name="VOUT0VSYNC"/>
<pin name="VOUT0AVID"/>
<pin name="VOUT0BCBC2"/>
<pin name="VOUT0BCBC3"/>
<pin name="VOUT0BCBC4"/>
<pin name="VOUT0BCBC5"/>
<pin name="VOUT0BCBC6"/>
<pin name="VOUT0BCBC7"/>
<pin name="VOUT0BCBC8"/>
<pin name="VOUT0BCBC9"/>
<pin name="VOUT0GYYC2"/>
<pin name="VOUT0GYYC3"/>
<pin name="VOUT0GYYC4"/>
<pin name="VOUT0GYYC5"/>
<pin name="VOUT0GYYC6"/>
<pin name="VOUT0GYYC7"/>
<pin name="VOUT0GYYC8"/>
<pin name="VOUT0GYYC9"/>
<pin name="VOUT0RCR2"/>
<pin name="VOUT0RCR3"/>
<pin name="VOUT0RCR4"/>
<pin name="VOUT0RCR5"/>
<pin name="VOUT0RCR6"/>
<pin name="VOUT0RCR7"/>
<pin name="VOUT0RCR8"/>
<pin name="VOUT0RCR9"/>
<pin name="USB0DRVVBUS"/>
<pin name="UART2TXD"/>
<pin name="UART0RXD"/>
<pin name="UART0TXD"/>
<pin name="UART0CTSN"/>
<pin name="UART0RTSN"/>
<pin name="UART0DCDN"/>
<pin name="UART0DSRN"/>
<pin name="UART0DTRN"/>
<pin name="UART0RIN"/>
<pin name="SPI0SCS1N"/>
<pin name="UART2RXD"/>
<pin name="SPI0SCS0N"/>
<pin name="SPI0SCLK"/>
<pin name="SPI0D1"/>
<pin name="SPI0D0"/>
<pin name="SPI1SCS0N"/>
<pin name="SPI1SCLK"/>
<pin name="SPI1D1"/>
<pin name="SPI1D0"/>
<pin name="I2C0SCL"/>
<pin name="I2C0SDA"/>
<pin name="DEVOSCWAKE"/>
<pin name="SD1CLK"/>
<pin name="SD1CMD"/>
<pin name="SD1DAT0"/>
<pin name="SD1DAT1SDIRQN"/>
<pin name="SD1DAT2SDRWN"/>
<pin name="SD1DAT3"/>
<pin name="SD0DAT3"/>
<pin name="SD0DAT2SDRWN"/>
<pin name="SD0DAT1SDIRQN"/>
<pin name="SD0DAT0"/>
<pin name="SD0CMD"/>
<pin name="SD0CLK"/>
<pin name="SD0DAT6"/>
<pin name="SD0DAT7"/>
<pin name="MCA1AXR1"/>
<pin name="MCA1AXR0"/>
<pin name="MCA1AFSX"/>
<pin name="MCA1ACLKX"/>
<pin name="MCA1AFSR"/>
<pin name="MCA1ACLKR"/>
<pin name="MCA0AXR3"/>
<pin name="MCA0AXR4"/>
<pin name="MCA0AXR5"/>
<pin name="MCA0ACLKX"/>
<pin name="MCA0AFSX"/>
<pin name="MCA0ACLKR"/>
<pin name="MCA0AXR2"/>
<pin name="MCA0AXR1"/>
<pin name="MCA0AXR0"/>
<pin name="MCA0AFSR"/>
<pin name="AUDCLKIN0"/>
<pin name="AUDCLKIN1"/>
<pin name="AUDCLKIN2"/>
<pin name="RESETN"/>
<pin name="NMIN"/>
<pin name="RSTOUTWDOUTN"/>
<pin name="CLKIN32"/>
<pin name="PORN" direction="in"/>
<pin name="TRSTN" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="DDR0DQS0N"/>
<pin name="DDR0DQS1N"/>
<pin name="DDR0DQS2N"/>
<pin name="DDR0DQS3N"/>
<pin name="VREFSSTLDDR0" direction="pas"/>
<pin name="VSSADEVOSC" direction="pwr"/>
<pin name="VSSAAUXOSC" direction="pwr"/>
<pin name="VSSAVDAC" direction="pwr"/>
<pin name="VSSACSI2@1" direction="pwr"/>
<pin name="VSSACSI2@2" direction="pwr"/>
<pin name="VSSAHDMI@1" direction="pwr"/>
<pin name="VSSAHDMI@2" direction="pwr"/>
<pin name="VSSAUSB@1" direction="pwr"/>
<pin name="VSSAUSB@2" direction="pwr"/>
<pin name="VSSAUSB@3" direction="pwr"/>
<pin name="RSV4" direction="pas"/>
<pin name="RSV5" direction="pas"/>
<pin name="CVDDARM@1" direction="pwr"/>
<pin name="CVDDARM@2" direction="pwr"/>
<pin name="CVDDARM@3" direction="pwr"/>
<pin name="CVDDARM@4" direction="pwr"/>
<pin name="CVDDARM@5" direction="pwr"/>
<pin name="CVDDARM@6" direction="pwr"/>
<pin name="CVDDHDVICP@1" direction="pwr"/>
<pin name="CVDDHDVICP@2" direction="pwr"/>
<pin name="CVDDHDVICP@3" direction="pwr"/>
<pin name="CVDDHDVICP@4" direction="pwr"/>
<pin name="CVDDHDVICP@5" direction="pwr"/>
<pin name="LDOCAPSERDESCLK" direction="pas"/>
<pin name="VDDAARMPLL1P8" direction="pwr"/>
<pin name="LDOCAPARM" direction="pas"/>
<pin name="LDOCAPHDVICP" direction="pas"/>
<pin name="VDDAAUDIOPLL1P8" direction="pwr"/>
<pin name="VDDAVDAC1P8" direction="pwr"/>
<pin name="VDDACSI21P8" direction="pwr"/>
<pin name="VDDADDRPLL1P8" direction="pwr"/>
<pin name="VDDAHDDAC1P1" direction="pwr"/>
<pin name="VDDAHDDAC1P8" direction="pwr"/>
<pin name="VDDAHDMI1P8" direction="pwr"/>
<pin name="VDDAL3L41P8" direction="pwr"/>
<pin name="VDDAHDVICPPLL1P8" direction="pwr"/>
<pin name="VDDAHDDACREF1P8" direction="pwr"/>
<pin name="VDDAVIDPLL1P8" direction="pwr"/>
<pin name="VDDAUSB01P8" direction="pwr"/>
<pin name="VDDAUSB11P8" direction="pwr"/>
<pin name="VDDAUSB3P3@1" direction="pwr"/>
<pin name="VDDAUSB3P3@2" direction="pwr"/>
<pin name="VDDAPCIE1P8" direction="pwr"/>
<pin name="RSV55" direction="pas"/>
<pin name="RSV54" direction="pas"/>
<pin name="LDOCAPARMRAM" direction="pas"/>
<pin name="LDOCAPRAM0" direction="pas"/>
<pin name="LDOCAPRAM1" direction="pas"/>
<pin name="LDOCAPRAM2" direction="pas"/>
<pin name="LDOCAPHDVICPRAM" direction="pas"/>
<pin name="VDDSOSC01P8" direction="pwr"/>
<pin name="VDDSOSC11P8" direction="pwr"/>
<pin name="VDDA1P8@1" direction="pwr"/>
<pin name="VDDA1P8@2" direction="pwr"/>
<pin name="VDDA1P8@3" direction="pwr"/>
<pin name="VDDA1P8@4" direction="pwr"/>
<pin name="VDDA1P8@5" direction="pwr"/>
<pin name="VDDA1P8@6" direction="pwr"/>
<pin name="VDDA1P8@7" direction="pwr"/>
<pin name="DVDDDDR0@1" direction="pwr"/>
<pin name="DVDDDDR0@2" direction="pwr"/>
<pin name="DVDDDDR0@3" direction="pwr"/>
<pin name="DVDDDDR0@4" direction="pwr"/>
<pin name="DVDDDDR0@5" direction="pwr"/>
<pin name="DVDDDDR0@6" direction="pwr"/>
<pin name="DVDDDDR0@7" direction="pwr"/>
<pin name="DVDDDDR0@8" direction="pwr"/>
<pin name="DVDDDDR0@9" direction="pwr"/>
<pin name="DVDDDDR0@10" direction="pwr"/>
<pin name="DVDDDDR0@11" direction="pwr"/>
<pin name="DVDDDDR0@12" direction="pwr"/>
<pin name="DVDDRGMII@1" direction="pwr"/>
<pin name="DVDDRGMII@2" direction="pwr"/>
<pin name="DVDDRGMII@3" direction="pwr"/>
<pin name="DVDDRGMII@4" direction="pwr"/>
<pin name="DVDDRGMII@5" direction="pwr"/>
<pin name="DVDDGPMC@1" direction="pwr"/>
<pin name="DVDDGPMC@2" direction="pwr"/>
<pin name="DVDDGPMC@3" direction="pwr"/>
<pin name="DVDDGPMC@4" direction="pwr"/>
<pin name="DVDDGPMC@5" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="DVDD@7" direction="pwr"/>
<pin name="DVDD@8" direction="pwr"/>
<pin name="DVDD@9" direction="pwr"/>
<pin name="DVDD@10" direction="pwr"/>
<pin name="DVDD@11" direction="pwr"/>
<pin name="DVDD@12" direction="pwr"/>
<pin name="DVDDC@1" direction="pwr"/>
<pin name="DVDDC@2" direction="pwr"/>
<pin name="DVDDC@3" direction="pwr"/>
<pin name="DVDDC@4" direction="pwr"/>
<pin name="DVDDC@5" direction="pwr"/>
<pin name="DVDDSD@1" direction="pwr"/>
<pin name="DVDDSD@2" direction="pwr"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="CVDD@7" direction="pwr"/>
<pin name="CVDD@8" direction="pwr"/>
<pin name="CVDD@9" direction="pwr"/>
<pin name="CVDD@10" direction="pwr"/>
<pin name="CVDD@11" direction="pwr"/>
<pin name="CVDD@12" direction="pwr"/>
<pin name="CVDD@13" direction="pwr"/>
<pin name="CVDD@14" direction="pwr"/>
<pin name="CVDD@15" direction="pwr"/>
<pin name="CVDD@16" direction="pwr"/>
<pin name="CVDD@17" direction="pwr"/>
<pin name="CVDD@18" direction="pwr"/>
<pin name="CVDD@19" direction="pwr"/>
<pin name="CVDD@20" direction="pwr"/>
<pin name="CVDD@21" direction="pwr"/>
<pin name="CVDD@22" direction="pwr"/>
<pin name="CVDD@23" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
<pin name="VSS@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="VSS@45" direction="pwr"/>
<pin name="VSS@46" direction="pwr"/>
<pin name="VSS@47" direction="pwr"/>
<pin name="VSS@48" direction="pwr"/>
<pin name="VSS@49" direction="pwr"/>
<pin name="VSS@50" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VSS@52" direction="pwr"/>
<pin name="VSS@53" direction="pwr"/>
<pin name="VSS@54" direction="pwr"/>
<pin name="VSS@55" direction="pwr"/>
<pin name="VSS@56" direction="pwr"/>
<pin name="VSS@57" direction="pwr"/>
<pin name="VSS@58" direction="pwr"/>
<pin name="VSS@59" direction="pwr"/>
<pin name="VSS@60" direction="pwr"/>
<pin name="VSS@61" direction="pwr"/>
<pin name="VSS@62" direction="pwr"/>
<pin name="VSS@63" direction="pwr"/>
<pin name="VSS@64" direction="pwr"/>
<pin name="VSS@65" direction="pwr"/>
<pin name="VSS@66" direction="pwr"/>
<pin name="VSS@67" direction="pwr"/>
<pin name="VSS@68" direction="pwr"/>
<pin name="VSS@69" direction="pwr"/>
<pin name="VSS@70" direction="pwr"/>
<pin name="VSS@71" direction="pwr"/>
<pin name="VSS@72" direction="pwr"/>
<pin name="VSS@73" direction="pwr"/>
<pin name="VSS@74" direction="pwr"/>
<pin name="VSS@75" direction="pwr"/>
<pin name="VSS@76" direction="pwr"/>
<pin name="VSS@77" direction="pwr"/>
<pin name="VSS@78" direction="pwr"/>
<pin name="VSS@79" direction="pwr"/>
<pin name="VSS@80" direction="pwr"/>
<pin name="VSS@81" direction="pwr"/>
<pin name="VSS@82" direction="pwr"/>
<pin name="VSS@83" direction="pwr"/>
<pin name="VSS@84" direction="pwr"/>
<pin name="VSS@85" direction="pwr"/>
<pin name="VSS@86" direction="pwr"/>
<pin name="VSS@87" direction="pwr"/>
<pin name="VSS@88" direction="pwr"/>
<pin name="VSS@89" direction="pwr"/>
<pin name="VSS@90" direction="pwr"/>
<pin name="VSS@91" direction="pwr"/>
<pin name="VSS@92" direction="pwr"/>
<pin name="VSS@93" direction="pwr"/>
<pin name="VSS@94" direction="pwr"/>
<pin name="VSS@95" direction="pwr"/>
<pin name="VSS@96" direction="pwr"/>
<pin name="VSS@97" direction="pwr"/>
<pin name="VSS@98" direction="pwr"/>
<pin name="VSS@99" direction="pwr"/>
<pin name="VSS@100" direction="pwr"/>
<pin name="VSS@101" direction="pwr"/>
<pin name="VSS@102" direction="pwr"/>
<pin name="VSS@103" direction="pwr"/>
<pin name="VSS@104" direction="pwr"/>
<pin name="VSS@105" direction="pwr"/>
</symbol>
<symbol name="DM385_A">
<pin name="MDIO"/>
<pin name="MDCLK"/>
<pin name="HDDACVSYNC"/>
<pin name="HDDACHSYNC"/>
<pin name="EMU1"/>
<pin name="EMU0"/>
<pin name="DEVOSCWAKE"/>
<pin name="AUDCLKIN0"/>
<pin name="AUDCLKIN1"/>
<pin name="AUDCLKIN2"/>
<pin name="RESETN"/>
<pin name="NMIN"/>
<pin name="RSTOUTWDOUTN"/>
<pin name="CLKIN32"/>
<pin name="PORN" direction="in"/>
<pin name="TRSTN" direction="in"/>
<pin name="TCLK" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDO" direction="out"/>
</symbol>
<symbol name="DM385_DDR">
<pin name="DDR0A13"/>
<pin name="DDR0A14"/>
<pin name="DDR0A1"/>
<pin name="DDR0A15"/>
<pin name="DDR0CS0N"/>
<pin name="DDR0ODT0"/>
<pin name="DDR0RST"/>
<pin name="DDR0CKE"/>
<pin name="DDR0RASN"/>
<pin name="DDR0CASN"/>
<pin name="DDR0A11"/>
<pin name="DDR0A0"/>
<pin name="DDR0A10"/>
<pin name="DDR0BA1"/>
<pin name="DDR0A7"/>
<pin name="DDR0A12"/>
<pin name="DDR0A2"/>
<pin name="DDR0A6"/>
<pin name="DDR0A9"/>
<pin name="DDR0A8"/>
<pin name="DDR0A4"/>
<pin name="DDR0A3"/>
<pin name="DDR0CLK"/>
<pin name="DDR0CLKN"/>
<pin name="DDR0A5"/>
<pin name="DDR0BA0"/>
<pin name="DDR0WEN"/>
<pin name="DDR0BA2"/>
<pin name="DDR0DQM3"/>
<pin name="DDR0DQM2"/>
<pin name="DDR0DQM1"/>
<pin name="DDR0DQM0"/>
<pin name="DDR0DQS3"/>
<pin name="DDR0DQS2"/>
<pin name="DDR0DQS1"/>
<pin name="DDR0DQS0"/>
<pin name="DDR0D31"/>
<pin name="DDR0D30"/>
<pin name="DDR0D29"/>
<pin name="DDR0D28"/>
<pin name="DDR0D27"/>
<pin name="DDR0D26"/>
<pin name="DDR0D25"/>
<pin name="DDR0D24"/>
<pin name="DDR0D23"/>
<pin name="DDR0D22"/>
<pin name="DDR0D21"/>
<pin name="DDR0D20"/>
<pin name="DDR0D19"/>
<pin name="DDR0D18"/>
<pin name="DDR0D17"/>
<pin name="DDR0D16"/>
<pin name="DDR0D15"/>
<pin name="DDR0D14"/>
<pin name="DDR0D13"/>
<pin name="DDR0D12"/>
<pin name="DDR0D11"/>
<pin name="DDR0D10"/>
<pin name="DDR0D9"/>
<pin name="DDR0D8"/>
<pin name="DDR0D7"/>
<pin name="DDR0D6"/>
<pin name="DDR0D5"/>
<pin name="DDR0D4"/>
<pin name="DDR0D3"/>
<pin name="DDR0D2"/>
<pin name="DDR0D1"/>
<pin name="DDR0D0"/>
<pin name="DDR0DQS0N"/>
<pin name="DDR0DQS1N"/>
<pin name="DDR0DQS2N"/>
<pin name="DDR0DQS3N"/>
<pin name="VREFSSTLDDR0" direction="pas"/>
</symbol>
<symbol name="DM385_EMA">
<pin name="EMAC0MTXEN_EMAC1RGRXD2"/>
<pin name="EMAC0MTXD7_EMAC1RGTXD3"/>
<pin name="EMAC0MTXD6_EMAC1RGRXD0"/>
<pin name="EMAC0MTXD5_EMAC1RGTXC"/>
<pin name="EMAC0MTXD4_EMAC1RGTXD2"/>
<pin name="EMAC0MTXD3_EMAC1RGTXD0"/>
<pin name="EMAC0MTXD2_EMAC1RGTXCTL"/>
<pin name="EMAC0MTXD1_EMAC1RGTXD1"/>
<pin name="EMAC0MTXD0_EMAC1RGRXD3"/>
<pin name="EMAC0GMTCLK_EMAC1RGRXC"/>
<pin name="EMAC0MRXDV_EMAC1RGRXD1"/>
<pin name="EMAC0MRXD7_EMAC0RGTXD1"/>
<pin name="EMAC0MRXD6_EMAC0RGTXD2"/>
<pin name="EMAC0MRXD5_EMAC0RGTXD3"/>
<pin name="EMAC0MRXD4_EMAC0RGRXD3"/>
<pin name="EMAC0MRXD3_EMAC1RGRXCTL"/>
<pin name="EMAC0MRXD2_EMAC0RGRXD1"/>
<pin name="EMAC0MRXD1_EMAC0RGRXD0"/>
<pin name="EMAC0MRCLK_EMAC0RGTXC"/>
<pin name="EMAC0MRXER_EMAC0RGTXCTL"/>
<pin name="EMAC0MRXD0_EMAC0RGTXD0"/>
<pin name="EMAC0MCRS_EMAC0RGRXD2"/>
<pin name="EMAC0MCOL_EMAC0RGRXCTL"/>
<pin name="EMAC0MTCLK_EMAC0RGRXC"/>
<pin name="EMACRMREFCLK"/>
</symbol>
<symbol name="DM385_MCA">
<pin name="MCA1AXR1"/>
<pin name="MCA1AXR0"/>
<pin name="MCA1AFSX"/>
<pin name="MCA1ACLKX"/>
<pin name="MCA1AFSR"/>
<pin name="MCA1ACLKR"/>
<pin name="MCA0AXR3"/>
<pin name="MCA0AXR4"/>
<pin name="MCA0AXR5"/>
<pin name="MCA0ACLKX"/>
<pin name="MCA0AFSX"/>
<pin name="MCA0ACLKR"/>
<pin name="MCA0AXR2"/>
<pin name="MCA0AXR1"/>
<pin name="MCA0AXR0"/>
<pin name="MCA0AFSR"/>
</symbol>
<symbol name="DM385_GPM">
<pin name="GPMCCS3N"/>
<pin name="GPMCCS4N"/>
<pin name="GPMCCS0N"/>
<pin name="GPMCCS1N"/>
<pin name="GPMCCS2N"/>
<pin name="GPMCCLK"/>
<pin name="GPMCADVNALE"/>
<pin name="GPMCOEREN"/>
<pin name="GPMCWEN"/>
<pin name="GPMCBE0NCLE"/>
<pin name="GPMCBE1N"/>
<pin name="GPMCWAIT0"/>
<pin name="GPMCD0"/>
<pin name="GPMCD1"/>
<pin name="GPMCD2"/>
<pin name="GPMCD3"/>
<pin name="GPMCD4"/>
<pin name="GPMCD5"/>
<pin name="GPMCD6"/>
<pin name="GPMCD7"/>
<pin name="GPMCD8"/>
<pin name="GPMCD9"/>
<pin name="GPMCD10"/>
<pin name="GPMCD11"/>
<pin name="GPMCD12"/>
<pin name="GPMCD13"/>
<pin name="GPMCD14"/>
<pin name="GPMCD15"/>
<pin name="GPMCA23"/>
<pin name="GPMCA22"/>
<pin name="GPMCA21"/>
<pin name="GPMCA20"/>
<pin name="GPMCA19"/>
<pin name="GPMCA18"/>
<pin name="GPMCA17"/>
<pin name="GPMCA16"/>
</symbol>
<symbol name="DM385_SD">
<pin name="SD2DAT7"/>
<pin name="SD2DAT6"/>
<pin name="SD2DAT5"/>
<pin name="SD2DAT4"/>
<pin name="SD2DAT3"/>
<pin name="SD2DAT2SDRWN"/>
<pin name="SD2SCLK"/>
<pin name="SD2DAT1SDIRQN"/>
<pin name="SD2DAT0"/>
<pin name="SD1CLK"/>
<pin name="SD1CMD"/>
<pin name="SD1DAT0"/>
<pin name="SD1DAT1SDIRQN"/>
<pin name="SD1DAT2SDRWN"/>
<pin name="SD1DAT3"/>
<pin name="SD0DAT3"/>
<pin name="SD0DAT2SDRWN"/>
<pin name="SD0DAT1SDIRQN"/>
<pin name="SD0DAT0"/>
<pin name="SD0CMD"/>
<pin name="SD0CLK"/>
<pin name="SD0DAT6"/>
<pin name="SD0DAT7"/>
</symbol>
<symbol name="DM385_SPI">
<pin name="SPI0SCS1N"/>
<pin name="SPI0SCS0N"/>
<pin name="SPI0SCLK"/>
<pin name="SPI0D1"/>
<pin name="SPI0D0"/>
<pin name="SPI1SCS0N"/>
<pin name="SPI1SCLK"/>
<pin name="SPI1D1"/>
<pin name="SPI1D0"/>
</symbol>
<symbol name="DM385_I2C">
<pin name="I2C1SCL"/>
<pin name="I2C1SDA"/>
<pin name="I2C0SCL"/>
<pin name="I2C0SDA"/>
</symbol>
<symbol name="DM385_UART">
<pin name="USB0DRVVBUS"/>
<pin name="UART2TXD"/>
<pin name="UART0RXD"/>
<pin name="UART0TXD"/>
<pin name="UART0CTSN"/>
<pin name="UART0RTSN"/>
<pin name="UART0DCDN"/>
<pin name="UART0DSRN"/>
<pin name="UART0DTRN"/>
<pin name="UART0RIN"/>
<pin name="UART2RXD"/>
</symbol>
<symbol name="DM385_LDO">
<pin name="LDOCAPSERDESCLK" direction="pas"/>
<pin name="LDOCAPARM" direction="pas"/>
<pin name="LDOCAPHDVICP" direction="pas"/>
<pin name="LDOCAPARMRAM" direction="pas"/>
<pin name="LDOCAPRAM0" direction="pas"/>
<pin name="LDOCAPRAM1" direction="pas"/>
<pin name="LDOCAPRAM2" direction="pas"/>
<pin name="LDOCAPHDVICPRAM" direction="pas"/>
</symbol>
<symbol name="DM385_VIN">
<pin name="VIN0BFLD"/>
<pin name="VIN0AFLD1"/>
<pin name="VIN0BDE"/>
<pin name="VIN0ADE1"/>
<pin name="VIN0AD23"/>
<pin name="VIN0AD22"/>
<pin name="VIN0AD21"/>
<pin name="VIN0AD20"/>
<pin name="VIN0AD19"/>
<pin name="VIN0AD18"/>
<pin name="VIN0AD17"/>
<pin name="VIN0AD16"/>
<pin name="VIN0BCLK"/>
<pin name="VIN0ADE"/>
<pin name="VIN0AFLD"/>
<pin name="VIN0ACLK"/>
<pin name="VIN0AHSYNC"/>
<pin name="VIN0AVSYNC"/>
<pin name="VIN0AD15BD7"/>
<pin name="VIN0AD14BD6"/>
<pin name="VIN0AD13BD5"/>
<pin name="VIN0AD12BD4"/>
<pin name="VIN0AD11BD3"/>
<pin name="VIN0AD10BD2"/>
<pin name="VIN0AD9BD1"/>
<pin name="VIN0AD8BD0"/>
<pin name="VIN0AD7"/>
<pin name="VIN0AD6"/>
<pin name="VIN0AD5"/>
<pin name="VIN0AD4"/>
<pin name="VIN0AD3"/>
<pin name="VIN0AD2"/>
<pin name="VIN0AD1"/>
<pin name="VIN0AD0"/>
</symbol>
<symbol name="DM385_VOUT">
<pin name="VOUT1BCBC2"/>
<pin name="VOUT1RCR2"/>
<pin name="VOUT1RCR3"/>
<pin name="VOUT1GYYC2"/>
<pin name="VOUT1RCR9"/>
<pin name="VOUT1RCR8"/>
<pin name="VOUT1RCR7"/>
<pin name="VOUT1RCR6"/>
<pin name="VOUT1RCR5"/>
<pin name="VOUT1RCR4"/>
<pin name="VOUT1GYYC9"/>
<pin name="VOUT1GYYC8"/>
<pin name="VOUT1GYYC7"/>
<pin name="VOUT1GYYC6"/>
<pin name="VOUT1GYYC5"/>
<pin name="VOUT1GYYC4"/>
<pin name="VOUT1GYYC3"/>
<pin name="VOUT1BCBC9"/>
<pin name="VOUT1BCBC8"/>
<pin name="VOUT1BCBC7"/>
<pin name="VOUT1BCBC6"/>
<pin name="VOUT1BCBC5"/>
<pin name="VOUT1BCBC4"/>
<pin name="VOUT1BCBC3"/>
<pin name="VOUT1AVID"/>
<pin name="VOUT1VSYNC"/>
<pin name="VOUT1HSYNC"/>
<pin name="VOUT1CLK"/>
<pin name="VOUT1FLD"/>
<pin name="VOUT1BCBC0"/>
<pin name="VOUT1BCBC1"/>
<pin name="VOUT1RCR0"/>
<pin name="VOUT1RCR1"/>
<pin name="VOUT1GYYC0"/>
<pin name="VOUT1GYYC1"/>
<pin name="VOUT0FLD"/>
<pin name="VOUT0CLK"/>
<pin name="VOUT0HSYNC"/>
<pin name="VOUT0VSYNC"/>
<pin name="VOUT0AVID"/>
<pin name="VOUT0BCBC2"/>
<pin name="VOUT0BCBC3"/>
<pin name="VOUT0BCBC4"/>
<pin name="VOUT0BCBC5"/>
<pin name="VOUT0BCBC6"/>
<pin name="VOUT0BCBC7"/>
<pin name="VOUT0BCBC8"/>
<pin name="VOUT0BCBC9"/>
<pin name="VOUT0GYYC2"/>
<pin name="VOUT0GYYC3"/>
<pin name="VOUT0GYYC4"/>
<pin name="VOUT0GYYC5"/>
<pin name="VOUT0GYYC6"/>
<pin name="VOUT0GYYC7"/>
<pin name="VOUT0GYYC8"/>
<pin name="VOUT0GYYC9"/>
<pin name="VOUT0RCR2"/>
<pin name="VOUT0RCR3"/>
<pin name="VOUT0RCR4"/>
<pin name="VOUT0RCR5"/>
<pin name="VOUT0RCR6"/>
<pin name="VOUT0RCR7"/>
<pin name="VOUT0RCR8"/>
<pin name="VOUT0RCR9"/>
</symbol>
<symbol name="DM385_CVDD">
<pin name="CVDDARM@1" direction="pwr"/>
<pin name="CVDDARM@2" direction="pwr"/>
<pin name="CVDDARM@3" direction="pwr"/>
<pin name="CVDDARM@4" direction="pwr"/>
<pin name="CVDDARM@5" direction="pwr"/>
<pin name="CVDDARM@6" direction="pwr"/>
<pin name="CVDDHDVICP@1" direction="pwr"/>
<pin name="CVDDHDVICP@2" direction="pwr"/>
<pin name="CVDDHDVICP@3" direction="pwr"/>
<pin name="CVDDHDVICP@4" direction="pwr"/>
<pin name="CVDDHDVICP@5" direction="pwr"/>
<pin name="CVDD@1" direction="pwr"/>
<pin name="CVDD@2" direction="pwr"/>
<pin name="CVDD@3" direction="pwr"/>
<pin name="CVDD@4" direction="pwr"/>
<pin name="CVDD@5" direction="pwr"/>
<pin name="CVDD@6" direction="pwr"/>
<pin name="CVDD@7" direction="pwr"/>
<pin name="CVDD@8" direction="pwr"/>
<pin name="CVDD@9" direction="pwr"/>
<pin name="CVDD@10" direction="pwr"/>
<pin name="CVDD@11" direction="pwr"/>
<pin name="CVDD@12" direction="pwr"/>
<pin name="CVDD@13" direction="pwr"/>
<pin name="CVDD@14" direction="pwr"/>
<pin name="CVDD@15" direction="pwr"/>
<pin name="CVDD@16" direction="pwr"/>
<pin name="CVDD@17" direction="pwr"/>
<pin name="CVDD@18" direction="pwr"/>
<pin name="CVDD@19" direction="pwr"/>
<pin name="CVDD@20" direction="pwr"/>
<pin name="CVDD@21" direction="pwr"/>
<pin name="CVDD@22" direction="pwr"/>
<pin name="CVDD@23" direction="pwr"/>
</symbol>
<symbol name="DM385_DVDD">
<pin name="DVDDDDR0@1" direction="pwr"/>
<pin name="DVDDDDR0@2" direction="pwr"/>
<pin name="DVDDDDR0@3" direction="pwr"/>
<pin name="DVDDDDR0@4" direction="pwr"/>
<pin name="DVDDDDR0@5" direction="pwr"/>
<pin name="DVDDDDR0@6" direction="pwr"/>
<pin name="DVDDDDR0@7" direction="pwr"/>
<pin name="DVDDDDR0@8" direction="pwr"/>
<pin name="DVDDDDR0@9" direction="pwr"/>
<pin name="DVDDDDR0@10" direction="pwr"/>
<pin name="DVDDDDR0@11" direction="pwr"/>
<pin name="DVDDDDR0@12" direction="pwr"/>
<pin name="DVDDRGMII@1" direction="pwr"/>
<pin name="DVDDRGMII@2" direction="pwr"/>
<pin name="DVDDRGMII@3" direction="pwr"/>
<pin name="DVDDRGMII@4" direction="pwr"/>
<pin name="DVDDRGMII@5" direction="pwr"/>
<pin name="DVDDGPMC@1" direction="pwr"/>
<pin name="DVDDGPMC@2" direction="pwr"/>
<pin name="DVDDGPMC@3" direction="pwr"/>
<pin name="DVDDGPMC@4" direction="pwr"/>
<pin name="DVDDGPMC@5" direction="pwr"/>
<pin name="DVDD@1" direction="pwr"/>
<pin name="DVDD@2" direction="pwr"/>
<pin name="DVDD@3" direction="pwr"/>
<pin name="DVDD@4" direction="pwr"/>
<pin name="DVDD@5" direction="pwr"/>
<pin name="DVDD@6" direction="pwr"/>
<pin name="DVDD@7" direction="pwr"/>
<pin name="DVDD@8" direction="pwr"/>
<pin name="DVDD@9" direction="pwr"/>
<pin name="DVDD@10" direction="pwr"/>
<pin name="DVDD@11" direction="pwr"/>
<pin name="DVDD@12" direction="pwr"/>
<pin name="DVDDC@1" direction="pwr"/>
<pin name="DVDDC@2" direction="pwr"/>
<pin name="DVDDC@3" direction="pwr"/>
<pin name="DVDDC@4" direction="pwr"/>
<pin name="DVDDC@5" direction="pwr"/>
<pin name="DVDDSD@1" direction="pwr"/>
<pin name="DVDDSD@2" direction="pwr"/>
</symbol>
<symbol name="DM385_VDD">
<pin name="VDDAARMPLL1P8" direction="pwr"/>
<pin name="VDDAAUDIOPLL1P8" direction="pwr"/>
<pin name="VDDAVDAC1P8" direction="pwr"/>
<pin name="VDDACSI21P8" direction="pwr"/>
<pin name="VDDADDRPLL1P8" direction="pwr"/>
<pin name="VDDAHDDAC1P1" direction="pwr"/>
<pin name="VDDAHDDAC1P8" direction="pwr"/>
<pin name="VDDAHDMI1P8" direction="pwr"/>
<pin name="VDDAL3L41P8" direction="pwr"/>
<pin name="VDDAHDVICPPLL1P8" direction="pwr"/>
<pin name="VDDAHDDACREF1P8" direction="pwr"/>
<pin name="VDDAVIDPLL1P8" direction="pwr"/>
<pin name="VDDAUSB01P8" direction="pwr"/>
<pin name="VDDAUSB11P8" direction="pwr"/>
<pin name="VDDAUSB3P3@1" direction="pwr"/>
<pin name="VDDAUSB3P3@2" direction="pwr"/>
<pin name="VDDAPCIE1P8" direction="pwr"/>
<pin name="VDDSOSC01P8" direction="pwr"/>
<pin name="VDDSOSC11P8" direction="pwr"/>
<pin name="VDDA1P8@1" direction="pwr"/>
<pin name="VDDA1P8@2" direction="pwr"/>
<pin name="VDDA1P8@3" direction="pwr"/>
<pin name="VDDA1P8@4" direction="pwr"/>
<pin name="VDDA1P8@5" direction="pwr"/>
<pin name="VDDA1P8@6" direction="pwr"/>
<pin name="VDDA1P8@7" direction="pwr"/>
</symbol>
<symbol name="DM385_VSS">
<pin name="VSSADEVOSC" direction="pwr"/>
<pin name="VSSAAUXOSC" direction="pwr"/>
<pin name="VSSAVDAC" direction="pwr"/>
<pin name="VSSACSI2@1" direction="pwr"/>
<pin name="VSSACSI2@2" direction="pwr"/>
<pin name="VSSAHDMI@1" direction="pwr"/>
<pin name="VSSAHDMI@2" direction="pwr"/>
<pin name="VSSAUSB@1" direction="pwr"/>
<pin name="VSSAUSB@2" direction="pwr"/>
<pin name="VSSAUSB@3" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="VSS@2" direction="pwr"/>
<pin name="VSS@3" direction="pwr"/>
<pin name="VSS@4" direction="pwr"/>
<pin name="VSS@5" direction="pwr"/>
<pin name="VSS@6" direction="pwr"/>
<pin name="VSS@7" direction="pwr"/>
<pin name="VSS@8" direction="pwr"/>
<pin name="VSS@9" direction="pwr"/>
<pin name="VSS@10" direction="pwr"/>
<pin name="VSS@11" direction="pwr"/>
<pin name="VSS@12" direction="pwr"/>
<pin name="VSS@13" direction="pwr"/>
<pin name="VSS@14" direction="pwr"/>
<pin name="VSS@15" direction="pwr"/>
<pin name="VSS@16" direction="pwr"/>
<pin name="VSS@17" direction="pwr"/>
<pin name="VSS@18" direction="pwr"/>
<pin name="VSS@19" direction="pwr"/>
<pin name="VSS@20" direction="pwr"/>
<pin name="VSS@21" direction="pwr"/>
<pin name="VSS@22" direction="pwr"/>
<pin name="VSS@23" direction="pwr"/>
<pin name="VSS@24" direction="pwr"/>
<pin name="VSS@25" direction="pwr"/>
<pin name="VSS@26" direction="pwr"/>
<pin name="VSS@27" direction="pwr"/>
<pin name="VSS@28" direction="pwr"/>
<pin name="VSS@29" direction="pwr"/>
<pin name="VSS@30" direction="pwr"/>
<pin name="VSS@31" direction="pwr"/>
<pin name="VSS@32" direction="pwr"/>
<pin name="VSS@33" direction="pwr"/>
<pin name="VSS@34" direction="pwr"/>
<pin name="VSS@35" direction="pwr"/>
<pin name="VSS@36" direction="pwr"/>
<pin name="VSS@37" direction="pwr"/>
<pin name="VSS@38" direction="pwr"/>
<pin name="VSS@39" direction="pwr"/>
<pin name="VSS@40" direction="pwr"/>
<pin name="VSS@41" direction="pwr"/>
<pin name="VSS@42" direction="pwr"/>
<pin name="VSS@43" direction="pwr"/>
<pin name="VSS@44" direction="pwr"/>
<pin name="VSS@45" direction="pwr"/>
<pin name="VSS@46" direction="pwr"/>
<pin name="VSS@47" direction="pwr"/>
<pin name="VSS@48" direction="pwr"/>
<pin name="VSS@49" direction="pwr"/>
<pin name="VSS@50" direction="pwr"/>
<pin name="VSS@51" direction="pwr"/>
<pin name="VSS@52" direction="pwr"/>
<pin name="VSS@53" direction="pwr"/>
<pin name="VSS@54" direction="pwr"/>
<pin name="VSS@55" direction="pwr"/>
<pin name="VSS@56" direction="pwr"/>
<pin name="VSS@57" direction="pwr"/>
<pin name="VSS@58" direction="pwr"/>
<pin name="VSS@59" direction="pwr"/>
<pin name="VSS@60" direction="pwr"/>
<pin name="VSS@61" direction="pwr"/>
<pin name="VSS@62" direction="pwr"/>
<pin name="VSS@63" direction="pwr"/>
<pin name="VSS@64" direction="pwr"/>
<pin name="VSS@65" direction="pwr"/>
<pin name="VSS@66" direction="pwr"/>
<pin name="VSS@67" direction="pwr"/>
<pin name="VSS@68" direction="pwr"/>
<pin name="VSS@69" direction="pwr"/>
<pin name="VSS@70" direction="pwr"/>
<pin name="VSS@71" direction="pwr"/>
<pin name="VSS@72" direction="pwr"/>
<pin name="VSS@73" direction="pwr"/>
<pin name="VSS@74" direction="pwr"/>
<pin name="VSS@75" direction="pwr"/>
<pin name="VSS@76" direction="pwr"/>
<pin name="VSS@77" direction="pwr"/>
<pin name="VSS@78" direction="pwr"/>
<pin name="VSS@79" direction="pwr"/>
<pin name="VSS@80" direction="pwr"/>
<pin name="VSS@81" direction="pwr"/>
<pin name="VSS@82" direction="pwr"/>
<pin name="VSS@83" direction="pwr"/>
<pin name="VSS@84" direction="pwr"/>
<pin name="VSS@85" direction="pwr"/>
<pin name="VSS@86" direction="pwr"/>
<pin name="VSS@87" direction="pwr"/>
<pin name="VSS@88" direction="pwr"/>
<pin name="VSS@89" direction="pwr"/>
<pin name="VSS@90" direction="pwr"/>
<pin name="VSS@91" direction="pwr"/>
<pin name="VSS@92" direction="pwr"/>
<pin name="VSS@93" direction="pwr"/>
<pin name="VSS@94" direction="pwr"/>
<pin name="VSS@95" direction="pwr"/>
<pin name="VSS@96" direction="pwr"/>
<pin name="VSS@97" direction="pwr"/>
<pin name="VSS@98" direction="pwr"/>
<pin name="VSS@99" direction="pwr"/>
<pin name="VSS@100" direction="pwr"/>
<pin name="VSS@101" direction="pwr"/>
<pin name="VSS@102" direction="pwr"/>
<pin name="VSS@103" direction="pwr"/>
<pin name="VSS@104" direction="pwr"/>
<pin name="VSS@105" direction="pwr"/>
</symbol>
<symbol name="DM385_RSV">
<pin name="RSV42"/>
<pin name="RSV4" direction="pas"/>
<pin name="RSV5" direction="pas"/>
<pin name="RSV55" direction="pas"/>
<pin name="RSV54" direction="pas"/>
</symbol>
<symbol name="ADS8684">
<pin name="GNDA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="AUX_IN" direction="in"/>
<pin name="NC@1" direction="nc"/>
<pin name="NC@2" direction="nc"/>
<pin name="NC@3" direction="nc"/>
<pin name="NC@4" direction="nc"/>
<pin name="AIN_0P" direction="in"/>
<pin name="AIN_0GND" direction="in"/>
<pin name="AIN_1P" direction="in"/>
<pin name="AIN_1GND" direction="in"/>
<pin name="AIN_2P" direction="in"/>
<pin name="AIN_2GND" direction="in"/>
<pin name="AIN_3P" direction="in"/>
<pin name="AIN_3GND" direction="in"/>
<pin name="NC@5" direction="nc"/>
<pin name="NC@6" direction="nc"/>
<pin name="NC@7" direction="nc"/>
<pin name="NC@8" direction="nc"/>
<pin name="GNDD" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="DNC" direction="nc"/>
<pin name="SDO"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="GNDA@1" direction="pwr"/>
<pin name="GNDA@2" direction="pwr"/>
<pin name="VDDA@1" direction="pwr"/>
<pin name="GNDA@3" direction="pwr"/>
<pin name="GNDA@4" direction="pwr"/>
<pin name="SDI" direction="in"/>
<pin name="!RST!/!PD" direction="in"/>
<pin name="DAISY" direction="in"/>
<pin name="!REFSEL" direction="in"/>
<pin name="REFIO"/>
<pin name="REFGND" direction="pwr"/>
<pin name="REFCAP" direction="out"/>
<pin name="AUX_GND" direction="in"/>
</symbol>
<symbol name="ADS8688">
<pin name="SDI" direction="in"/>
<pin name="!RST!/!PD" direction="in"/>
<pin name="DAISY" direction="in"/>
<pin name="!REFSEL" direction="in"/>
<pin name="REFIO"/>
<pin name="REFGND" direction="pwr"/>
<pin name="GNDA" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="AUX_IN" direction="in"/>
<pin name="AIN_0P" direction="in"/>
<pin name="AIN_0GND" direction="in"/>
<pin name="AIN_1P" direction="in"/>
<pin name="AIN_1GND" direction="in"/>
<pin name="AIN_2P" direction="in"/>
<pin name="AIN_2GND" direction="in"/>
<pin name="AIN_3P" direction="in"/>
<pin name="AIN_3GND" direction="in"/>
<pin name="GNDA@1" direction="pwr"/>
<pin name="GNDA@2" direction="pwr"/>
<pin name="VDDA@1" direction="pwr"/>
<pin name="GNDD" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="DNC" direction="nc"/>
<pin name="SDO"/>
<pin name="SCLK" direction="in"/>
<pin name="!CS" direction="in"/>
<pin name="REFCAP" direction="out"/>
<pin name="AIN_6P" direction="in"/>
<pin name="AIN_6GND" direction="in"/>
<pin name="AIN_7P" direction="in"/>
<pin name="AIN_7GND" direction="in"/>
<pin name="AIN_4GND" direction="in"/>
<pin name="AIN_4P" direction="in"/>
<pin name="AIN_5GND" direction="in"/>
<pin name="AIN_5P" direction="in"/>
<pin name="AUX_GND" direction="in"/>
<pin name="GNDA@3" direction="pwr"/>
<pin name="GNDA@4" direction="pwr"/>
</symbol>
<symbol name="ADS7042">
<pin name="AINM" direction="in"/>
<pin name="AINP" direction="in"/>
<pin name="SDO"/>
<pin name="SCLK" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VDDA" direction="pwr"/>
<pin name="VDDD" direction="pwr"/>
<pin name="!SC" direction="in"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BQ2054PN" prefix="U">
<description>&lt;b&gt;CHARGE MANAGEMENT IC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BQ2054"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="BAT" pad="3"/>
<connect gate="G$1" pin="ICOMP" pad="5"/>
<connect gate="G$1" pin="ICTL" pad="2"/>
<connect gate="G$1" pin="ITERM" pad="6"/>
<connect gate="G$1" pin="LCOM" pad="11"/>
<connect gate="G$1" pin="LED1" pad="15"/>
<connect gate="G$1" pin="LED2/DSL" pad="16"/>
<connect gate="G$1" pin="LED3" pad="10"/>
<connect gate="G$1" pin="MOD" pad="14"/>
<connect gate="G$1" pin="SNS" pad="7"/>
<connect gate="G$1" pin="TM" pad="1"/>
<connect gate="G$1" pin="TPWM" pad="9"/>
<connect gate="G$1" pin="TS" pad="8"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VCOMP" pad="4"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="BQ2054PN"/>
<attribute name="OC_FARNELL" value="8407789"/>
<attribute name="OC_NEWARK" value="74C7582"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2054SN" prefix="U">
<description>&lt;b&gt;CHARGE MANAGEMENT IC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BQ2054"/>
</gates>
<devices>
<device name="" package="SO-16">
<connects>
<connect gate="G$1" pin="BAT" pad="3"/>
<connect gate="G$1" pin="ICOMP" pad="5"/>
<connect gate="G$1" pin="ICTL" pad="2"/>
<connect gate="G$1" pin="ITERM" pad="6"/>
<connect gate="G$1" pin="LCOM" pad="11"/>
<connect gate="G$1" pin="LED1" pad="15"/>
<connect gate="G$1" pin="LED2/DSL" pad="16"/>
<connect gate="G$1" pin="LED3" pad="10"/>
<connect gate="G$1" pin="MOD" pad="14"/>
<connect gate="G$1" pin="SNS" pad="7"/>
<connect gate="G$1" pin="TM" pad="1"/>
<connect gate="G$1" pin="TPWM" pad="9"/>
<connect gate="G$1" pin="TS" pad="8"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VCOMP" pad="4"/>
<connect gate="G$1" pin="VSS" pad="12"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="BQ2054SN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="74C7583"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2058T" prefix="U">
<description>&lt;b&gt;CHARGE MANAGEMENT IC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BQ2058"/>
</gates>
<devices>
<device name="" package="SO-16">
<connects>
<connect gate="G$1" pin="B1N" pad="8"/>
<connect gate="G$1" pin="B1P" pad="9"/>
<connect gate="G$1" pin="B2N" pad="5"/>
<connect gate="G$1" pin="B2N1" pad="6"/>
<connect gate="G$1" pin="B2N2" pad="7"/>
<connect gate="G$1" pin="CHG" pad="1"/>
<connect gate="G$1" pin="CSH" pad="10"/>
<connect gate="G$1" pin="CSL" pad="4"/>
<connect gate="G$1" pin="CTRL" pad="2"/>
<connect gate="G$1" pin="DSG" pad="16"/>
<connect gate="G$1" pin="OCD" pad="12"/>
<connect gate="G$1" pin="OVD" pad="13"/>
<connect gate="G$1" pin="UVD" pad="14"/>
<connect gate="G$1" pin="VCC" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="15"/>
<connect gate="G$1" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2002TS" prefix="IC">
<description>&lt;b&gt;CHARGE MANAGEMENT IC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BQ2002"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="BAT" pad="3"/>
<connect gate="G$1" pin="CC" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="INH" pad="7"/>
<connect gate="G$1" pin="LED/" pad="2"/>
<connect gate="G$1" pin="TM" pad="1"/>
<connect gate="G$1" pin="TS" pad="5"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="BQ2002TSN"/>
<attribute name="OC_FARNELL" value="1564910"/>
<attribute name="OC_NEWARK" value="74C7527"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2002TP" prefix="IC">
<description>&lt;b&gt;CHARGE MANAGEMENT IC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BQ2002"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="BAT" pad="3"/>
<connect gate="G$1" pin="CC" pad="8"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="INH" pad="7"/>
<connect gate="G$1" pin="LED/" pad="2"/>
<connect gate="G$1" pin="TM" pad="1"/>
<connect gate="G$1" pin="TS" pad="5"/>
<connect gate="G$1" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="BQ2002TPN"/>
<attribute name="OC_FARNELL" value="8409668"/>
<attribute name="OC_NEWARK" value="74C7526"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="320C5402" prefix="IC" uservalue="yes">
<description>&lt;b&gt;DSP DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="320C5402"/>
</gates>
<devices>
<device name="" package="PQFP144">
<connects>
<connect gate="G$1" pin="!BIO" pad="31"/>
<connect gate="G$1" pin="!DS" pad="21"/>
<connect gate="G$1" pin="!HAS" pad="13"/>
<connect gate="G$1" pin="!HCS" pad="17"/>
<connect gate="G$1" pin="!HDS1" pad="127"/>
<connect gate="G$1" pin="!HDS2" pad="129"/>
<connect gate="G$1" pin="!HINT" pad="51"/>
<connect gate="G$1" pin="!HOLD" pad="30"/>
<connect gate="G$1" pin="!HOLDA" pad="28"/>
<connect gate="G$1" pin="!IACK" pad="61"/>
<connect gate="G$1" pin="!IAQ" pad="29"/>
<connect gate="G$1" pin="!INT0" pad="64"/>
<connect gate="G$1" pin="!INT1" pad="65"/>
<connect gate="G$1" pin="!INT2" pad="66"/>
<connect gate="G$1" pin="!INT3" pad="67"/>
<connect gate="G$1" pin="!IOSTRB" pad="25"/>
<connect gate="G$1" pin="!IS" pad="22"/>
<connect gate="G$1" pin="!MSC" pad="26"/>
<connect gate="G$1" pin="!MSTRB" pad="24"/>
<connect gate="G$1" pin="!NMI" pad="63"/>
<connect gate="G$1" pin="!PS" pad="20"/>
<connect gate="G$1" pin="!RS" pad="98"/>
<connect gate="G$1" pin="!TRST" pad="87"/>
<connect gate="G$1" pin="A0" pad="131"/>
<connect gate="G$1" pin="A1" pad="132"/>
<connect gate="G$1" pin="A10" pad="5"/>
<connect gate="G$1" pin="A11" pad="7"/>
<connect gate="G$1" pin="A12" pad="8"/>
<connect gate="G$1" pin="A13" pad="9"/>
<connect gate="G$1" pin="A14" pad="10"/>
<connect gate="G$1" pin="A15" pad="11"/>
<connect gate="G$1" pin="A16" pad="105"/>
<connect gate="G$1" pin="A17" pad="107"/>
<connect gate="G$1" pin="A18" pad="108"/>
<connect gate="G$1" pin="A19" pad="109"/>
<connect gate="G$1" pin="A2" pad="133"/>
<connect gate="G$1" pin="A3" pad="134"/>
<connect gate="G$1" pin="A4" pad="136"/>
<connect gate="G$1" pin="A5" pad="137"/>
<connect gate="G$1" pin="A6" pad="138"/>
<connect gate="G$1" pin="A7" pad="139"/>
<connect gate="G$1" pin="A8" pad="140"/>
<connect gate="G$1" pin="A9" pad="141"/>
<connect gate="G$1" pin="BCLKR0" pad="41"/>
<connect gate="G$1" pin="BCLKR1" pad="42"/>
<connect gate="G$1" pin="BCLKX0" pad="48"/>
<connect gate="G$1" pin="BCLKX1" pad="49"/>
<connect gate="G$1" pin="BDR0" pad="45"/>
<connect gate="G$1" pin="BDR1" pad="47"/>
<connect gate="G$1" pin="BDX0" pad="59"/>
<connect gate="G$1" pin="BDX1" pad="60"/>
<connect gate="G$1" pin="BFSR0" pad="43"/>
<connect gate="G$1" pin="BFSR1" pad="44"/>
<connect gate="G$1" pin="BFSX0" pad="53"/>
<connect gate="G$1" pin="BFSX1" pad="54"/>
<connect gate="G$1" pin="CLKMD1" pad="77"/>
<connect gate="G$1" pin="CLKMD2" pad="78"/>
<connect gate="G$1" pin="CLKMD3" pad="79"/>
<connect gate="G$1" pin="CLKOUT" pad="94"/>
<connect gate="G$1" pin="CVDD@1" pad="16"/>
<connect gate="G$1" pin="CVDD@2" pad="52"/>
<connect gate="G$1" pin="CVDD@3" pad="68"/>
<connect gate="G$1" pin="CVDD@4" pad="91"/>
<connect gate="G$1" pin="CVDD@5" pad="125"/>
<connect gate="G$1" pin="CVDD@6" pad="142"/>
<connect gate="G$1" pin="D0" pad="99"/>
<connect gate="G$1" pin="D1" pad="100"/>
<connect gate="G$1" pin="D10" pad="117"/>
<connect gate="G$1" pin="D11" pad="118"/>
<connect gate="G$1" pin="D12" pad="119"/>
<connect gate="G$1" pin="D13" pad="121"/>
<connect gate="G$1" pin="D14" pad="122"/>
<connect gate="G$1" pin="D15" pad="123"/>
<connect gate="G$1" pin="D2" pad="101"/>
<connect gate="G$1" pin="D3" pad="102"/>
<connect gate="G$1" pin="D4" pad="103"/>
<connect gate="G$1" pin="D5" pad="104"/>
<connect gate="G$1" pin="D6" pad="113"/>
<connect gate="G$1" pin="D7" pad="114"/>
<connect gate="G$1" pin="D8" pad="115"/>
<connect gate="G$1" pin="D9" pad="116"/>
<connect gate="G$1" pin="DVDD@1" pad="4"/>
<connect gate="G$1" pin="DVDD@2" pad="33"/>
<connect gate="G$1" pin="DVDD@3" pad="56"/>
<connect gate="G$1" pin="DVDD@4" pad="75"/>
<connect gate="G$1" pin="DVDD@5" pad="112"/>
<connect gate="G$1" pin="DVDD@6" pad="130"/>
<connect gate="G$1" pin="EMU0" pad="83"/>
<connect gate="G$1" pin="EMU1/!OFF" pad="84"/>
<connect gate="G$1" pin="HBIL" pad="62"/>
<connect gate="G$1" pin="HCNTL0" pad="39"/>
<connect gate="G$1" pin="HCNTL1" pad="46"/>
<connect gate="G$1" pin="HD0" pad="58"/>
<connect gate="G$1" pin="HD1" pad="69"/>
<connect gate="G$1" pin="HD2" pad="81"/>
<connect gate="G$1" pin="HD3" pad="95"/>
<connect gate="G$1" pin="HD4" pad="120"/>
<connect gate="G$1" pin="HD5" pad="124"/>
<connect gate="G$1" pin="HD6" pad="135"/>
<connect gate="G$1" pin="HD7" pad="6"/>
<connect gate="G$1" pin="HPIENA" pad="92"/>
<connect gate="G$1" pin="HR/!W" pad="18"/>
<connect gate="G$1" pin="HRDY" pad="55"/>
<connect gate="G$1" pin="MP/!MC" pad="32"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC10" pad="72"/>
<connect gate="G$1" pin="NC11" pad="73"/>
<connect gate="G$1" pin="NC12" pad="74"/>
<connect gate="G$1" pin="NC13" pad="80"/>
<connect gate="G$1" pin="NC14" pad="90"/>
<connect gate="G$1" pin="NC15" pad="110"/>
<connect gate="G$1" pin="NC16" pad="126"/>
<connect gate="G$1" pin="NC17" pad="143"/>
<connect gate="G$1" pin="NC18" pad="144"/>
<connect gate="G$1" pin="NC2" pad="2"/>
<connect gate="G$1" pin="NC3" pad="12"/>
<connect gate="G$1" pin="NC4" pad="15"/>
<connect gate="G$1" pin="NC5" pad="35"/>
<connect gate="G$1" pin="NC6" pad="36"/>
<connect gate="G$1" pin="NC7" pad="37"/>
<connect gate="G$1" pin="NC8" pad="38"/>
<connect gate="G$1" pin="NC9" pad="71"/>
<connect gate="G$1" pin="R/!W" pad="23"/>
<connect gate="G$1" pin="READY" pad="19"/>
<connect gate="G$1" pin="TCK" pad="88"/>
<connect gate="G$1" pin="TDI" pad="86"/>
<connect gate="G$1" pin="TDO" pad="85"/>
<connect gate="G$1" pin="TMS" pad="89"/>
<connect gate="G$1" pin="TOUT0" pad="82"/>
<connect gate="G$1" pin="VSS@1" pad="3"/>
<connect gate="G$1" pin="VSS@10" pad="106"/>
<connect gate="G$1" pin="VSS@11" pad="111"/>
<connect gate="G$1" pin="VSS@12" pad="128"/>
<connect gate="G$1" pin="VSS@2" pad="14"/>
<connect gate="G$1" pin="VSS@3" pad="34"/>
<connect gate="G$1" pin="VSS@4" pad="40"/>
<connect gate="G$1" pin="VSS@5" pad="50"/>
<connect gate="G$1" pin="VSS@6" pad="57"/>
<connect gate="G$1" pin="VSS@7" pad="70"/>
<connect gate="G$1" pin="VSS@8" pad="76"/>
<connect gate="G$1" pin="VSS@9" pad="93"/>
<connect gate="G$1" pin="X1" pad="96"/>
<connect gate="G$1" pin="X2/CLKIN" pad="97"/>
<connect gate="G$1" pin="XF" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLV320AC56" prefix="IC">
<description>&lt;b&gt;VOICE BAND AUDIO PROCESSOR&lt;/b&gt;</description>
<gates>
<gate name="N" symbol="TLV320AC"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL20">
<connects>
<connect gate="N" pin="!EARMUTE" pad="10"/>
<connect gate="N" pin="!LINSEL" pad="15"/>
<connect gate="N" pin="!MICMUTE" pad="6"/>
<connect gate="N" pin="!PDN" pad="1"/>
<connect gate="N" pin="!TSX-DCLKX" pad="14"/>
<connect gate="N" pin="CLK" pad="11"/>
<connect gate="N" pin="DCLKR" pad="7"/>
<connect gate="N" pin="DIN" pad="8"/>
<connect gate="N" pin="DOUT" pad="13"/>
<connect gate="N" pin="EARA" pad="2"/>
<connect gate="N" pin="EARB" pad="3"/>
<connect gate="N" pin="EARGS" pad="4"/>
<connect gate="N" pin="FSR" pad="9"/>
<connect gate="N" pin="FSX" pad="12"/>
<connect gate="N" pin="MICBIAS" pad="20"/>
<connect gate="N" pin="MICGS" pad="19"/>
<connect gate="N" pin="MICIN" pad="18"/>
<connect gate="N" pin="VMID" pad="17"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLV320ACDW" prefix="IC">
<description>&lt;b&gt;DSP DEVICE&lt;/b&gt;</description>
<gates>
<gate name="DW" symbol="TLV320AC"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="SO-20DW">
<connects>
<connect gate="DW" pin="!EARMUTE" pad="10"/>
<connect gate="DW" pin="!LINSEL" pad="15"/>
<connect gate="DW" pin="!MICMUTE" pad="6"/>
<connect gate="DW" pin="!PDN" pad="1"/>
<connect gate="DW" pin="!TSX-DCLKX" pad="14"/>
<connect gate="DW" pin="CLK" pad="11"/>
<connect gate="DW" pin="DCLKR" pad="7"/>
<connect gate="DW" pin="DIN" pad="8"/>
<connect gate="DW" pin="DOUT" pad="13"/>
<connect gate="DW" pin="EARA" pad="2"/>
<connect gate="DW" pin="EARB" pad="3"/>
<connect gate="DW" pin="EARGS" pad="4"/>
<connect gate="DW" pin="FSR" pad="9"/>
<connect gate="DW" pin="FSX" pad="12"/>
<connect gate="DW" pin="MICBIAS" pad="20"/>
<connect gate="DW" pin="MICGS" pad="19"/>
<connect gate="DW" pin="MICIN" pad="18"/>
<connect gate="DW" pin="VMID" pad="17"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLV320AC-P" prefix="IC">
<description>&lt;b&gt;DSP DEVICE&lt;/b&gt;</description>
<gates>
<gate name="PT" symbol="TLV320AC"/>
<gate name="A" symbol="AVCCGND"/>
<gate name="D" symbol="DVCCGND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC47" symbol="NC"/>
<gate name="NC48" symbol="NC"/>
</gates>
<devices>
<device name="" package="PQFP48">
<connects>
<connect gate="A" pin="AGND" pad="34"/>
<connect gate="A" pin="AVCC" pad="4"/>
<connect gate="D" pin="DGND" pad="27"/>
<connect gate="D" pin="DVCC" pad="9"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="10"/>
<connect gate="NC12" pin="NC" pad="12"/>
<connect gate="NC13" pin="NC" pad="13"/>
<connect gate="NC18" pin="NC" pad="18"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC23" pin="NC" pad="23"/>
<connect gate="NC24" pin="NC" pad="24"/>
<connect gate="NC25" pin="NC" pad="25"/>
<connect gate="NC28" pin="NC" pad="28"/>
<connect gate="NC29" pin="NC" pad="29"/>
<connect gate="NC3" pin="NC" pad="3"/>
<connect gate="NC30" pin="NC" pad="30"/>
<connect gate="NC31" pin="NC" pad="31"/>
<connect gate="NC32" pin="NC" pad="32"/>
<connect gate="NC33" pin="NC" pad="33"/>
<connect gate="NC35" pin="NC" pad="35"/>
<connect gate="NC37" pin="NC" pad="37"/>
<connect gate="NC38" pin="NC" pad="38"/>
<connect gate="NC39" pin="NC" pad="39"/>
<connect gate="NC47" pin="NC" pad="47"/>
<connect gate="NC48" pin="NC" pad="48"/>
<connect gate="NC5" pin="NC" pad="5"/>
<connect gate="NC6" pin="NC" pad="6"/>
<connect gate="NC7" pin="NC" pad="7"/>
<connect gate="NC8" pin="NC" pad="8"/>
<connect gate="PT" pin="!EARMUTE" pad="17"/>
<connect gate="PT" pin="!LINSEL" pad="26"/>
<connect gate="PT" pin="!MICMUTE" pad="11"/>
<connect gate="PT" pin="!PDN" pad="43"/>
<connect gate="PT" pin="!TSX-DCLKX" pad="22"/>
<connect gate="PT" pin="CLK" pad="19"/>
<connect gate="PT" pin="DCLKR" pad="14"/>
<connect gate="PT" pin="DIN" pad="15"/>
<connect gate="PT" pin="DOUT" pad="21"/>
<connect gate="PT" pin="EARA" pad="44"/>
<connect gate="PT" pin="EARB" pad="45"/>
<connect gate="PT" pin="EARGS" pad="46"/>
<connect gate="PT" pin="FSR" pad="16"/>
<connect gate="PT" pin="FSX" pad="20"/>
<connect gate="PT" pin="MICBIAS" pad="42"/>
<connect gate="PT" pin="MICGS" pad="41"/>
<connect gate="PT" pin="MICIN" pad="40"/>
<connect gate="PT" pin="VMID" pad="36"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="320C5402-B" prefix="IC" uservalue="yes">
<description>&lt;b&gt;DSP DEVICE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="320C54-B"/>
<gate name="P" symbol="320PWR"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
</gates>
<devices>
<device name="" package="PQFP144">
<connects>
<connect gate="A" pin="!BIO" pad="31"/>
<connect gate="A" pin="!DS" pad="21"/>
<connect gate="A" pin="!HAS" pad="13"/>
<connect gate="A" pin="!HCS" pad="17"/>
<connect gate="A" pin="!HDS1" pad="127"/>
<connect gate="A" pin="!HDS2" pad="129"/>
<connect gate="A" pin="!HINT" pad="51"/>
<connect gate="A" pin="!HOLD" pad="30"/>
<connect gate="A" pin="!HOLDA" pad="28"/>
<connect gate="A" pin="!IACK" pad="61"/>
<connect gate="A" pin="!IAQ" pad="29"/>
<connect gate="A" pin="!INT0" pad="64"/>
<connect gate="A" pin="!INT1" pad="65"/>
<connect gate="A" pin="!INT2" pad="66"/>
<connect gate="A" pin="!INT3" pad="67"/>
<connect gate="A" pin="!IOSTRB" pad="25"/>
<connect gate="A" pin="!IS" pad="22"/>
<connect gate="A" pin="!MSC" pad="26"/>
<connect gate="A" pin="!MSTRB" pad="24"/>
<connect gate="A" pin="!NMI" pad="63"/>
<connect gate="A" pin="!PS" pad="20"/>
<connect gate="A" pin="!RS" pad="98"/>
<connect gate="A" pin="!TRST" pad="87"/>
<connect gate="A" pin="A0" pad="131"/>
<connect gate="A" pin="A1" pad="132"/>
<connect gate="A" pin="A10" pad="5"/>
<connect gate="A" pin="A11" pad="7"/>
<connect gate="A" pin="A12" pad="8"/>
<connect gate="A" pin="A13" pad="9"/>
<connect gate="A" pin="A14" pad="10"/>
<connect gate="A" pin="A15" pad="11"/>
<connect gate="A" pin="A16" pad="105"/>
<connect gate="A" pin="A17" pad="107"/>
<connect gate="A" pin="A18" pad="108"/>
<connect gate="A" pin="A19" pad="109"/>
<connect gate="A" pin="A2" pad="133"/>
<connect gate="A" pin="A3" pad="134"/>
<connect gate="A" pin="A4" pad="136"/>
<connect gate="A" pin="A5" pad="137"/>
<connect gate="A" pin="A6" pad="138"/>
<connect gate="A" pin="A7" pad="139"/>
<connect gate="A" pin="A8" pad="140"/>
<connect gate="A" pin="A9" pad="141"/>
<connect gate="A" pin="BCLKR0" pad="41"/>
<connect gate="A" pin="BCLKR1" pad="42"/>
<connect gate="A" pin="BCLKX0" pad="48"/>
<connect gate="A" pin="BCLKX1" pad="49"/>
<connect gate="A" pin="BDR0" pad="45"/>
<connect gate="A" pin="BDR1" pad="47"/>
<connect gate="A" pin="BDX0" pad="59"/>
<connect gate="A" pin="BDX1" pad="60"/>
<connect gate="A" pin="BFSR0" pad="43"/>
<connect gate="A" pin="BFSR1" pad="44"/>
<connect gate="A" pin="BFSX0" pad="53"/>
<connect gate="A" pin="BFSX1" pad="54"/>
<connect gate="A" pin="CLKMD1" pad="77"/>
<connect gate="A" pin="CLKMD2" pad="78"/>
<connect gate="A" pin="CLKMD3" pad="79"/>
<connect gate="A" pin="CLKOUT" pad="94"/>
<connect gate="A" pin="D0" pad="99"/>
<connect gate="A" pin="D1" pad="100"/>
<connect gate="A" pin="D10" pad="117"/>
<connect gate="A" pin="D11" pad="118"/>
<connect gate="A" pin="D12" pad="119"/>
<connect gate="A" pin="D13" pad="121"/>
<connect gate="A" pin="D14" pad="122"/>
<connect gate="A" pin="D15" pad="123"/>
<connect gate="A" pin="D2" pad="101"/>
<connect gate="A" pin="D3" pad="102"/>
<connect gate="A" pin="D4" pad="103"/>
<connect gate="A" pin="D5" pad="104"/>
<connect gate="A" pin="D6" pad="113"/>
<connect gate="A" pin="D7" pad="114"/>
<connect gate="A" pin="D8" pad="115"/>
<connect gate="A" pin="D9" pad="116"/>
<connect gate="A" pin="EMU0" pad="83"/>
<connect gate="A" pin="EMU1/!OFF" pad="84"/>
<connect gate="A" pin="HBIL" pad="62"/>
<connect gate="A" pin="HCNTL0" pad="39"/>
<connect gate="A" pin="HCNTL1" pad="46"/>
<connect gate="A" pin="HD0" pad="58"/>
<connect gate="A" pin="HD1" pad="69"/>
<connect gate="A" pin="HD2" pad="81"/>
<connect gate="A" pin="HD3" pad="95"/>
<connect gate="A" pin="HD4" pad="120"/>
<connect gate="A" pin="HD5" pad="124"/>
<connect gate="A" pin="HD6" pad="135"/>
<connect gate="A" pin="HD7" pad="6"/>
<connect gate="A" pin="HPIENA" pad="92"/>
<connect gate="A" pin="HR/!W" pad="18"/>
<connect gate="A" pin="HRDY" pad="55"/>
<connect gate="A" pin="MP/!MC" pad="32"/>
<connect gate="A" pin="R/!W" pad="23"/>
<connect gate="A" pin="READY" pad="19"/>
<connect gate="A" pin="TCK" pad="88"/>
<connect gate="A" pin="TDI" pad="86"/>
<connect gate="A" pin="TDO" pad="85"/>
<connect gate="A" pin="TMS" pad="89"/>
<connect gate="A" pin="TOUT0" pad="82"/>
<connect gate="A" pin="X1" pad="96"/>
<connect gate="A" pin="X2/CLKIN" pad="97"/>
<connect gate="A" pin="XF" pad="27"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="72"/>
<connect gate="NC11" pin="NC" pad="73"/>
<connect gate="NC12" pin="NC" pad="74"/>
<connect gate="NC13" pin="NC" pad="80"/>
<connect gate="NC14" pin="NC" pad="90"/>
<connect gate="NC15" pin="NC" pad="110"/>
<connect gate="NC16" pin="NC" pad="126"/>
<connect gate="NC17" pin="NC" pad="143"/>
<connect gate="NC18" pin="NC" pad="144"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC3" pin="NC" pad="12"/>
<connect gate="NC4" pin="NC" pad="15"/>
<connect gate="NC5" pin="NC" pad="35"/>
<connect gate="NC6" pin="NC" pad="36"/>
<connect gate="NC7" pin="NC" pad="37"/>
<connect gate="NC8" pin="NC" pad="38"/>
<connect gate="NC9" pin="NC" pad="71"/>
<connect gate="P" pin="CVDD@1" pad="16"/>
<connect gate="P" pin="CVDD@2" pad="52"/>
<connect gate="P" pin="CVDD@3" pad="68"/>
<connect gate="P" pin="CVDD@4" pad="91"/>
<connect gate="P" pin="CVDD@5" pad="125"/>
<connect gate="P" pin="CVDD@6" pad="142"/>
<connect gate="P" pin="DVDD@1" pad="4"/>
<connect gate="P" pin="DVDD@2" pad="33"/>
<connect gate="P" pin="DVDD@3" pad="56"/>
<connect gate="P" pin="DVDD@4" pad="75"/>
<connect gate="P" pin="DVDD@5" pad="112"/>
<connect gate="P" pin="DVDD@6" pad="130"/>
<connect gate="P" pin="VSS@1" pad="3"/>
<connect gate="P" pin="VSS@10" pad="106"/>
<connect gate="P" pin="VSS@11" pad="111"/>
<connect gate="P" pin="VSS@12" pad="128"/>
<connect gate="P" pin="VSS@2" pad="14"/>
<connect gate="P" pin="VSS@3" pad="34"/>
<connect gate="P" pin="VSS@4" pad="40"/>
<connect gate="P" pin="VSS@5" pad="50"/>
<connect gate="P" pin="VSS@6" pad="57"/>
<connect gate="P" pin="VSS@7" pad="70"/>
<connect gate="P" pin="VSS@8" pad="76"/>
<connect gate="P" pin="VSS@9" pad="93"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L293E" prefix="IC">
<description>&lt;b&gt;TI DEVICE&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="L293E"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="1-2EN" pad="1"/>
<connect gate="G$1" pin="1A" pad="2"/>
<connect gate="G$1" pin="1Y" pad="3"/>
<connect gate="G$1" pin="2A" pad="7"/>
<connect gate="G$1" pin="2Y" pad="6"/>
<connect gate="G$1" pin="3-4EN" pad="9"/>
<connect gate="G$1" pin="3A" pad="10"/>
<connect gate="G$1" pin="3Y" pad="11"/>
<connect gate="G$1" pin="4A" pad="15"/>
<connect gate="G$1" pin="4Y" pad="14"/>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="GND3" pad="13"/>
<connect gate="G$1" pin="GND4" pad="12"/>
<connect gate="G$1" pin="VCC1" pad="16"/>
<connect gate="G$1" pin="VCC2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="MPN" value="L293E"/>
<attribute name="OC_FARNELL" value="1467711"/>
<attribute name="OC_NEWARK" value="89K0732"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2000TPN" prefix="IC">
<description>&lt;b&gt;CHARGE MANAGEMENT IC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BQ2000"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="!LED" pad="3"/>
<connect gate="G$1" pin="BAT" pad="4"/>
<connect gate="G$1" pin="MOD" pad="8"/>
<connect gate="G$1" pin="RC" pad="6"/>
<connect gate="G$1" pin="SNS" pad="1"/>
<connect gate="G$1" pin="TS" pad="5"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="BQ2000TPN-B5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="74C7505"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2000TSN" prefix="IC">
<description>&lt;b&gt;CHARGE MANAGEMENT IC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BQ2000"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="!LED" pad="3"/>
<connect gate="G$1" pin="BAT" pad="4"/>
<connect gate="G$1" pin="MOD" pad="8"/>
<connect gate="G$1" pin="RC" pad="6"/>
<connect gate="G$1" pin="SNS" pad="1"/>
<connect gate="G$1" pin="TS" pad="5"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="BQ2000TSN-B5"/>
<attribute name="OC_FARNELL" value="1212295"/>
<attribute name="OC_NEWARK" value="74C7508"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2000TTS" prefix="IC">
<description>&lt;b&gt;CHARGE MANAGEMENT IC&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="BQ2000"/>
</gates>
<devices>
<device name="" package="TSSOP8">
<connects>
<connect gate="G$1" pin="!LED" pad="3"/>
<connect gate="G$1" pin="BAT" pad="4"/>
<connect gate="G$1" pin="MOD" pad="8"/>
<connect gate="G$1" pin="RC" pad="6"/>
<connect gate="G$1" pin="SNS" pad="1"/>
<connect gate="G$1" pin="TS" pad="5"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC1526Q" prefix="IC">
<description>&lt;b&gt;PULSE WIDTH MODULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UC1526"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
</gates>
<devices>
<device name="" package="PLCC20">
<connects>
<connect gate="G$1" pin="!RESET" pad="6"/>
<connect gate="G$1" pin="!SHDOWN" pad="9"/>
<connect gate="G$1" pin="!SYNC" pad="13"/>
<connect gate="G$1" pin="+ERR" pad="2"/>
<connect gate="G$1" pin="+SENSE" pad="8"/>
<connect gate="G$1" pin="+VIN" pad="19"/>
<connect gate="G$1" pin="-ERR" pad="3"/>
<connect gate="G$1" pin="-SENSE" pad="7"/>
<connect gate="G$1" pin="COMP" pad="4"/>
<connect gate="G$1" pin="CSS" pad="5"/>
<connect gate="G$1" pin="CT" pad="11"/>
<connect gate="G$1" pin="GND" pad="17"/>
<connect gate="G$1" pin="OUTA" pad="14"/>
<connect gate="G$1" pin="OUTB" pad="18"/>
<connect gate="G$1" pin="RD" pad="12"/>
<connect gate="G$1" pin="RT" pad="10"/>
<connect gate="G$1" pin="VC" pad="15"/>
<connect gate="G$1" pin="VREF" pad="20"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC2" pin="NC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC1526DW" prefix="IC">
<description>&lt;b&gt;PULSE WIDTH MODULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UC1526"/>
</gates>
<devices>
<device name="" package="SO-18DW">
<connects>
<connect gate="G$1" pin="!RESET" pad="5"/>
<connect gate="G$1" pin="!SHDOWN" pad="8"/>
<connect gate="G$1" pin="!SYNC" pad="12"/>
<connect gate="G$1" pin="+ERR" pad="1"/>
<connect gate="G$1" pin="+SENSE" pad="7"/>
<connect gate="G$1" pin="+VIN" pad="17"/>
<connect gate="G$1" pin="-ERR" pad="2"/>
<connect gate="G$1" pin="-SENSE" pad="6"/>
<connect gate="G$1" pin="COMP" pad="3"/>
<connect gate="G$1" pin="CSS" pad="4"/>
<connect gate="G$1" pin="CT" pad="10"/>
<connect gate="G$1" pin="GND" pad="15"/>
<connect gate="G$1" pin="OUTA" pad="13"/>
<connect gate="G$1" pin="OUTB" pad="16"/>
<connect gate="G$1" pin="RD" pad="11"/>
<connect gate="G$1" pin="RT" pad="9"/>
<connect gate="G$1" pin="VC" pad="14"/>
<connect gate="G$1" pin="VREF" pad="18"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC1843DW" prefix="IC">
<description>&lt;b&gt;PULSE WIDTH MODULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UC1843"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
</gates>
<devices>
<device name="" package="SO-14DW">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="PWRGND" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="7"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="VC" pad="11"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VFB" pad="3"/>
<connect gate="G$1" pin="VREF" pad="14"/>
<connect gate="NC1" pin="NC" pad="2"/>
<connect gate="NC2" pin="NC" pad="4"/>
<connect gate="NC3" pin="NC" pad="6"/>
<connect gate="NC4" pin="NC" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC1843D8" prefix="IC">
<description>&lt;b&gt;PULSE WIDTH MODULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UC1843-8"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="SENSE" pad="3"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
<connect gate="G$1" pin="VREF" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="UC1843AMDREP"/>
<attribute name="OC_FARNELL" value="1755515"/>
<attribute name="OC_NEWARK" value="46M1388"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC1843Q" prefix="IC">
<description>&lt;b&gt;PULSE WIDTH MODULATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="UC1843"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
</gates>
<devices>
<device name="" package="PLCC20">
<connects>
<connect gate="G$1" pin="COMP" pad="2"/>
<connect gate="G$1" pin="GND" pad="13"/>
<connect gate="G$1" pin="OUT" pad="15"/>
<connect gate="G$1" pin="PWRGND" pad="12"/>
<connect gate="G$1" pin="RT/CT" pad="10"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
<connect gate="G$1" pin="VC" pad="17"/>
<connect gate="G$1" pin="VCC" pad="18"/>
<connect gate="G$1" pin="VFB" pad="5"/>
<connect gate="G$1" pin="VREF" pad="20"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="19"/>
<connect gate="NC2" pin="NC" pad="3"/>
<connect gate="NC3" pin="NC" pad="4"/>
<connect gate="NC4" pin="NC" pad="6"/>
<connect gate="NC5" pin="NC" pad="8"/>
<connect gate="NC6" pin="NC" pad="9"/>
<connect gate="NC7" pin="NC" pad="11"/>
<connect gate="NC8" pin="NC" pad="14"/>
<connect gate="NC9" pin="NC" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSL230*" prefix="IC">
<description>&lt;b&gt;PROGRAMMABLE LIGHT TO FREQUENCY CONVERTER&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TSL230"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="" package="DIL08-OPTO">
<connects>
<connect gate="G$1" pin="!OE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="S0" pad="1"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="7"/>
<connect gate="G$1" pin="S3" pad="8"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TSL230RP-LF"/>
<attribute name="OC_FARNELL" value="1182355"/>
<attribute name="OC_NEWARK" value="24M8654"/>
</technology>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF1706" prefix="IC">
<description>&lt;b&gt;Stereo, 24-Bit, 192kHz 8x Oversampling Digital Interpolation Filter&lt;/b&gt;&lt;p&gt;
www.ti.com df1706.pdf</description>
<gates>
<gate name="A" symbol="DF1706"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="A" pin="!MUTE" pad="15"/>
<connect gate="A" pin="!RST" pad="14"/>
<connect gate="A" pin="BCKIN" pad="2"/>
<connect gate="A" pin="BCKO" pad="26"/>
<connect gate="A" pin="CLKO" pad="9"/>
<connect gate="A" pin="DEM" pad="16"/>
<connect gate="A" pin="DGND" pad="8"/>
<connect gate="A" pin="DIN" pad="1"/>
<connect gate="A" pin="DOL" pad="24"/>
<connect gate="A" pin="DOR" pad="23"/>
<connect gate="A" pin="IIS" pad="3"/>
<connect gate="A" pin="IW0" pad="4"/>
<connect gate="A" pin="IW1" pad="5"/>
<connect gate="A" pin="LRCIN" pad="28"/>
<connect gate="A" pin="MC/LRIP" pad="12"/>
<connect gate="A" pin="MD/CKO" pad="11"/>
<connect gate="A" pin="ML/RESV" pad="13"/>
<connect gate="A" pin="MODE" pad="10"/>
<connect gate="A" pin="OSS" pad="21"/>
<connect gate="A" pin="OW0" pad="19"/>
<connect gate="A" pin="OW1" pad="20"/>
<connect gate="A" pin="SF0" pad="17"/>
<connect gate="A" pin="SF1" pad="18"/>
<connect gate="A" pin="SRO" pad="27"/>
<connect gate="A" pin="VDD" pad="22"/>
<connect gate="A" pin="WCKO" pad="25"/>
<connect gate="A" pin="XTI" pad="6"/>
<connect gate="A" pin="XTO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DF1706EG4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="66K1929"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM29*" prefix="IC">
<description>&lt;b&gt;STEREO AUDIO CODEC WITH USB INTERFACE&lt;/b&gt;&lt;p&gt;
SINGLE-ENDED ANALOG INPUT/OUTPUT AND S/PDIF</description>
<gates>
<gate name="A" symbol="PCM2900"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="A" pin="!SSPND" pad="28"/>
<connect gate="A" pin="AGNDC" pad="11"/>
<connect gate="A" pin="AGNDP" pad="18"/>
<connect gate="A" pin="AGNDX" pad="22"/>
<connect gate="A" pin="D+" pad="1"/>
<connect gate="A" pin="D-" pad="2"/>
<connect gate="A" pin="DGND" pad="26"/>
<connect gate="A" pin="DGNDU" pad="4"/>
<connect gate="A" pin="HID0" pad="5"/>
<connect gate="A" pin="HID1" pad="6"/>
<connect gate="A" pin="HID2" pad="7"/>
<connect gate="A" pin="SEL0" pad="8"/>
<connect gate="A" pin="SEL1" pad="9"/>
<connect gate="A" pin="TEST0" pad="24"/>
<connect gate="A" pin="TEST1" pad="25"/>
<connect gate="A" pin="VBUS" pad="3"/>
<connect gate="A" pin="VCCCI" pad="10"/>
<connect gate="A" pin="VCCP1I" pad="17"/>
<connect gate="A" pin="VCCP2I" pad="19"/>
<connect gate="A" pin="VCCXI" pad="23"/>
<connect gate="A" pin="VCOM" pad="14"/>
<connect gate="A" pin="VDDI" pad="27"/>
<connect gate="A" pin="VINL" pad="12"/>
<connect gate="A" pin="VINR" pad="13"/>
<connect gate="A" pin="VOUTL" pad="16"/>
<connect gate="A" pin="VOUTR" pad="15"/>
<connect gate="A" pin="XTI" pad="21"/>
<connect gate="A" pin="XTO" pad="20"/>
</connects>
<technologies>
<technology name="00E">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PCM2900E"/>
<attribute name="OC_FARNELL" value="1207086"/>
<attribute name="OC_NEWARK" value="75C5376"/>
</technology>
<technology name="04DB">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM2904DB"/>
<attribute name="OC_FARNELL" value="1207091"/>
<attribute name="OC_NEWARK" value="75C5386"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM290*" prefix="IC">
<description>&lt;b&gt;STEREO AUDIO CODEC WITH USB INTERFACE&lt;/b&gt;&lt;p&gt;
SINGLE-ENDED ANALOG INPUT/OUTPUT AND S/PDIF</description>
<gates>
<gate name="A" symbol="PCM2902"/>
</gates>
<devices>
<device name="" package="SSOP28DB">
<connects>
<connect gate="A" pin="!SSPND" pad="28"/>
<connect gate="A" pin="AGNDC" pad="11"/>
<connect gate="A" pin="AGNDP" pad="18"/>
<connect gate="A" pin="AGNDX" pad="22"/>
<connect gate="A" pin="D+" pad="1"/>
<connect gate="A" pin="D-" pad="2"/>
<connect gate="A" pin="DGND" pad="26"/>
<connect gate="A" pin="DGNDU" pad="4"/>
<connect gate="A" pin="DIN" pad="24"/>
<connect gate="A" pin="DOUT" pad="25"/>
<connect gate="A" pin="HID0" pad="5"/>
<connect gate="A" pin="HID1" pad="6"/>
<connect gate="A" pin="HID2" pad="7"/>
<connect gate="A" pin="SEL0" pad="8"/>
<connect gate="A" pin="SEL1" pad="9"/>
<connect gate="A" pin="VBUS" pad="3"/>
<connect gate="A" pin="VCCCI" pad="10"/>
<connect gate="A" pin="VCCP1I" pad="17"/>
<connect gate="A" pin="VCCP2I" pad="19"/>
<connect gate="A" pin="VCCXI" pad="23"/>
<connect gate="A" pin="VCOM" pad="14"/>
<connect gate="A" pin="VDDI" pad="27"/>
<connect gate="A" pin="VINL" pad="12"/>
<connect gate="A" pin="VINR" pad="13"/>
<connect gate="A" pin="VOUTL" pad="16"/>
<connect gate="A" pin="VOUTR" pad="15"/>
<connect gate="A" pin="XTI" pad="21"/>
<connect gate="A" pin="XTO" pad="20"/>
</connects>
<technologies>
<technology name="2E">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM2902E"/>
<attribute name="OC_FARNELL" value="1207089"/>
<attribute name="OC_NEWARK" value="75C5380"/>
</technology>
<technology name="6DB">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM2906DB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="83C7389"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PLL1700*" prefix="IC">
<description>&lt;b&gt;MULTI-CLOCK GENERATOR&lt;/b&gt;&lt;p&gt;
GENERATED AUDIO SYSTEM CLOCK&lt;br&gt;
Phase Lock Loop (PLL).</description>
<gates>
<gate name="A" symbol="PLL1700"/>
</gates>
<devices>
<device name="" package="SSOP20">
<connects>
<connect gate="A" pin="!MCKO" pad="11"/>
<connect gate="A" pin="DNGP" pad="7"/>
<connect gate="A" pin="GND" pad="4"/>
<connect gate="A" pin="GNDB" pad="15"/>
<connect gate="A" pin="MCKO" pad="10"/>
<connect gate="A" pin="MD/FS0" pad="19"/>
<connect gate="A" pin="MD/FS1" pad="20"/>
<connect gate="A" pin="ML/SR0" pad="1"/>
<connect gate="A" pin="MODE" pad="2"/>
<connect gate="A" pin="RST" pad="18"/>
<connect gate="A" pin="RSV" pad="9"/>
<connect gate="A" pin="SCKO1" pad="12"/>
<connect gate="A" pin="SCKO2" pad="14"/>
<connect gate="A" pin="SCKO3" pad="17"/>
<connect gate="A" pin="SCKO4" pad="13"/>
<connect gate="A" pin="VDD" pad="3"/>
<connect gate="A" pin="VDDB" pad="16"/>
<connect gate="A" pin="VDDP" pad="8"/>
<connect gate="A" pin="XT1" pad="6"/>
<connect gate="A" pin="XT2" pad="5"/>
</connects>
<technologies>
<technology name="E">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PLL1700E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="36K3452"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAS3001" prefix="IC">
<description>&lt;b&gt;TAS3001C Digital Audio Processor&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="A" symbol="TAS3001"/>
</gates>
<devices>
<device name="" package="PSO28">
<connects>
<connect gate="A" pin="!RES" pad="19"/>
<connect gate="A" pin="AVDD_PLL" pad="13"/>
<connect gate="A" pin="AVSS_PLL" pad="12"/>
<connect gate="A" pin="CAP_PLL" pad="14"/>
<connect gate="A" pin="CS1" pad="28"/>
<connect gate="A" pin="CS2" pad="1"/>
<connect gate="A" pin="DVDD" pad="3"/>
<connect gate="A" pin="DVSS" pad="2"/>
<connect gate="A" pin="LRCLK" pad="10"/>
<connect gate="A" pin="LRCLKO" pad="23"/>
<connect gate="A" pin="MCLK" pad="9"/>
<connect gate="A" pin="NC1" pad="17"/>
<connect gate="A" pin="NC2" pad="18"/>
<connect gate="A" pin="NC3" pad="20"/>
<connect gate="A" pin="NC4" pad="21"/>
<connect gate="A" pin="NC5" pad="22"/>
<connect gate="A" pin="NC6" pad="25"/>
<connect gate="A" pin="NC7" pad="26"/>
<connect gate="A" pin="POWDN" pad="16"/>
<connect gate="A" pin="RESERVED1" pad="15"/>
<connect gate="A" pin="RESERVED2" pad="27"/>
<connect gate="A" pin="SCL" pad="5"/>
<connect gate="A" pin="SCLK" pad="11"/>
<connect gate="A" pin="SCLKO" pad="24"/>
<connect gate="A" pin="SDA" pad="4"/>
<connect gate="A" pin="SDIN1" pad="6"/>
<connect gate="A" pin="SDIN2" pad="7"/>
<connect gate="A" pin="SDOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAS3002" prefix="IC">
<description>&lt;b&gt;Digital Audio Processor with Codec&lt;/b&gt;&lt;p&gt;
www.ti.com; tas3002.pdf</description>
<gates>
<gate name="A" symbol="TAS3002"/>
</gates>
<devices>
<device name="" package="PQFP48">
<connects>
<connect gate="A" pin="!INPA" pad="5"/>
<connect gate="A" pin="!RES" pad="6"/>
<connect gate="A" pin="AINLM" pad="46"/>
<connect gate="A" pin="AINLP" pad="47"/>
<connect gate="A" pin="AINRM" pad="43"/>
<connect gate="A" pin="AINRP" pad="42"/>
<connect gate="A" pin="ALLPASS" pad="27"/>
<connect gate="A" pin="AOUTL" pad="39"/>
<connect gate="A" pin="AUTOR" pad="37"/>
<connect gate="A" pin="AVDD" pad="35"/>
<connect gate="A" pin="AVSS" pad="4"/>
<connect gate="A" pin="AVSS(REF)" pad="3"/>
<connect gate="A" pin="CAP_PLL" pad="10"/>
<connect gate="A" pin="CLKSEL" pad="11"/>
<connect gate="A" pin="CS1" pad="7"/>
<connect gate="A" pin="DVDD" pad="17"/>
<connect gate="A" pin="DVSS" pad="18"/>
<connect gate="A" pin="GPI0" pad="28"/>
<connect gate="A" pin="GPI1" pad="29"/>
<connect gate="A" pin="GPI2" pad="30"/>
<connect gate="A" pin="GPI3" pad="31"/>
<connect gate="A" pin="GPI4" pad="32"/>
<connect gate="A" pin="GPI5" pad="33"/>
<connect gate="A" pin="IFM/!S" pad="21"/>
<connect gate="A" pin="LINA" pad="1"/>
<connect gate="A" pin="LINB" pad="48"/>
<connect gate="A" pin="LRCLK/O" pad="19"/>
<connect gate="A" pin="MCLKO" pad="12"/>
<connect gate="A" pin="NC1" pad="34"/>
<connect gate="A" pin="NC2" pad="36"/>
<connect gate="A" pin="PWR_DN" pad="8"/>
<connect gate="A" pin="RINA" pad="40"/>
<connect gate="A" pin="RINB" pad="41"/>
<connect gate="A" pin="SCL" pad="15"/>
<connect gate="A" pin="SCLK/O" pad="20"/>
<connect gate="A" pin="SDA" pad="16"/>
<connect gate="A" pin="SDIN1" pad="22"/>
<connect gate="A" pin="SDIN2" pad="23"/>
<connect gate="A" pin="SDOUT0" pad="25"/>
<connect gate="A" pin="SDOUT1" pad="26"/>
<connect gate="A" pin="SDOUT2" pad="24"/>
<connect gate="A" pin="TEST" pad="9"/>
<connect gate="A" pin="VCOM" pad="38"/>
<connect gate="A" pin="VREFM" pad="45"/>
<connect gate="A" pin="VREFP" pad="44"/>
<connect gate="A" pin="VRFILT" pad="2"/>
<connect gate="A" pin="XTALI" pad="13"/>
<connect gate="A" pin="XTALO" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TAS3002PFB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="76C5960"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320VC5402" prefix="IC">
<description>&lt;b&gt;Fixed-Point Digital Signal Processor&lt;/b&gt;&lt;p&gt;
Source: tms320vc5402.pdf</description>
<gates>
<gate name="G$1" symbol="TMS320VC5402"/>
</gates>
<devices>
<device name="PGE" package="PQFP144">
<connects>
<connect gate="G$1" pin="!BIO" pad="31"/>
<connect gate="G$1" pin="!DS" pad="21"/>
<connect gate="G$1" pin="!HAS" pad="13"/>
<connect gate="G$1" pin="!HCS" pad="17"/>
<connect gate="G$1" pin="!HDS1" pad="127"/>
<connect gate="G$1" pin="!HDS2" pad="129"/>
<connect gate="G$1" pin="!HINT!/OUT1" pad="51"/>
<connect gate="G$1" pin="!HOLD" pad="30"/>
<connect gate="G$1" pin="!HOLDA" pad="28"/>
<connect gate="G$1" pin="!IACK" pad="61"/>
<connect gate="G$1" pin="!IAQ" pad="29"/>
<connect gate="G$1" pin="!INT0" pad="64"/>
<connect gate="G$1" pin="!INT1" pad="65"/>
<connect gate="G$1" pin="!INT2" pad="66"/>
<connect gate="G$1" pin="!INT3" pad="67"/>
<connect gate="G$1" pin="!IOSTRB" pad="25"/>
<connect gate="G$1" pin="!IS" pad="22"/>
<connect gate="G$1" pin="!MSC" pad="26"/>
<connect gate="G$1" pin="!MSTRB" pad="24"/>
<connect gate="G$1" pin="!NMI" pad="63"/>
<connect gate="G$1" pin="!PS" pad="20"/>
<connect gate="G$1" pin="!RS" pad="98"/>
<connect gate="G$1" pin="!TRST" pad="87"/>
<connect gate="G$1" pin="A0" pad="131"/>
<connect gate="G$1" pin="A1" pad="132"/>
<connect gate="G$1" pin="A10" pad="5"/>
<connect gate="G$1" pin="A11" pad="7"/>
<connect gate="G$1" pin="A12" pad="8"/>
<connect gate="G$1" pin="A13" pad="9"/>
<connect gate="G$1" pin="A14" pad="10"/>
<connect gate="G$1" pin="A15" pad="11"/>
<connect gate="G$1" pin="A16" pad="105"/>
<connect gate="G$1" pin="A17" pad="107"/>
<connect gate="G$1" pin="A18" pad="108"/>
<connect gate="G$1" pin="A19" pad="109"/>
<connect gate="G$1" pin="A2" pad="133"/>
<connect gate="G$1" pin="A3" pad="134"/>
<connect gate="G$1" pin="A4" pad="136"/>
<connect gate="G$1" pin="A5" pad="137"/>
<connect gate="G$1" pin="A6" pad="138"/>
<connect gate="G$1" pin="A7" pad="139"/>
<connect gate="G$1" pin="A8" pad="140"/>
<connect gate="G$1" pin="A9" pad="141"/>
<connect gate="G$1" pin="BCLKR0" pad="41"/>
<connect gate="G$1" pin="BCLKR1" pad="42"/>
<connect gate="G$1" pin="BCLKX0" pad="48"/>
<connect gate="G$1" pin="BCLKX1" pad="49"/>
<connect gate="G$1" pin="BDR0" pad="45"/>
<connect gate="G$1" pin="BDR1" pad="47"/>
<connect gate="G$1" pin="BDX0" pad="59"/>
<connect gate="G$1" pin="BDX1" pad="60"/>
<connect gate="G$1" pin="BFSR0" pad="43"/>
<connect gate="G$1" pin="BFSR1" pad="44"/>
<connect gate="G$1" pin="BFSX0" pad="53"/>
<connect gate="G$1" pin="BFSX1" pad="54"/>
<connect gate="G$1" pin="CLKMD1" pad="77"/>
<connect gate="G$1" pin="CLKMD2" pad="78"/>
<connect gate="G$1" pin="CLKMD3" pad="79"/>
<connect gate="G$1" pin="CLKOUT" pad="94"/>
<connect gate="G$1" pin="CVDD@1" pad="16"/>
<connect gate="G$1" pin="CVDD@2" pad="52"/>
<connect gate="G$1" pin="CVDD@3" pad="68"/>
<connect gate="G$1" pin="CVDD@4" pad="91"/>
<connect gate="G$1" pin="CVDD@5" pad="125"/>
<connect gate="G$1" pin="CVDD@6" pad="142"/>
<connect gate="G$1" pin="D0" pad="99"/>
<connect gate="G$1" pin="D1" pad="100"/>
<connect gate="G$1" pin="D10" pad="117"/>
<connect gate="G$1" pin="D11" pad="118"/>
<connect gate="G$1" pin="D12" pad="119"/>
<connect gate="G$1" pin="D13" pad="121"/>
<connect gate="G$1" pin="D14" pad="122"/>
<connect gate="G$1" pin="D15" pad="123"/>
<connect gate="G$1" pin="D2" pad="101"/>
<connect gate="G$1" pin="D3" pad="102"/>
<connect gate="G$1" pin="D4" pad="103"/>
<connect gate="G$1" pin="D5" pad="104"/>
<connect gate="G$1" pin="D6" pad="113"/>
<connect gate="G$1" pin="D7" pad="114"/>
<connect gate="G$1" pin="D8" pad="115"/>
<connect gate="G$1" pin="D9" pad="116"/>
<connect gate="G$1" pin="DVDD@0" pad="4"/>
<connect gate="G$1" pin="DVDD@1" pad="56"/>
<connect gate="G$1" pin="DVDD@2" pad="33"/>
<connect gate="G$1" pin="DVDD@3" pad="75"/>
<connect gate="G$1" pin="DVDD@4" pad="112"/>
<connect gate="G$1" pin="DVDD@5" pad="130"/>
<connect gate="G$1" pin="EMU0" pad="83"/>
<connect gate="G$1" pin="EMU1" pad="84"/>
<connect gate="G$1" pin="HBIL" pad="62"/>
<connect gate="G$1" pin="HCNTL0" pad="39"/>
<connect gate="G$1" pin="HCNTL1" pad="46"/>
<connect gate="G$1" pin="HD0" pad="58"/>
<connect gate="G$1" pin="HD1" pad="69"/>
<connect gate="G$1" pin="HD2" pad="81"/>
<connect gate="G$1" pin="HD3" pad="95"/>
<connect gate="G$1" pin="HD4" pad="120"/>
<connect gate="G$1" pin="HD5" pad="124"/>
<connect gate="G$1" pin="HD6" pad="135"/>
<connect gate="G$1" pin="HD7" pad="6"/>
<connect gate="G$1" pin="HPIENA" pad="92"/>
<connect gate="G$1" pin="HR/!W" pad="18"/>
<connect gate="G$1" pin="HRDY" pad="55"/>
<connect gate="G$1" pin="MP/!MC" pad="32"/>
<connect gate="G$1" pin="NC@1" pad="1"/>
<connect gate="G$1" pin="NC@10" pad="72"/>
<connect gate="G$1" pin="NC@11" pad="73"/>
<connect gate="G$1" pin="NC@12" pad="74"/>
<connect gate="G$1" pin="NC@13" pad="80"/>
<connect gate="G$1" pin="NC@14" pad="90"/>
<connect gate="G$1" pin="NC@15" pad="110"/>
<connect gate="G$1" pin="NC@16" pad="126"/>
<connect gate="G$1" pin="NC@17" pad="143"/>
<connect gate="G$1" pin="NC@18" pad="144"/>
<connect gate="G$1" pin="NC@2" pad="2"/>
<connect gate="G$1" pin="NC@3" pad="12"/>
<connect gate="G$1" pin="NC@4" pad="15"/>
<connect gate="G$1" pin="NC@5" pad="35"/>
<connect gate="G$1" pin="NC@6" pad="36"/>
<connect gate="G$1" pin="NC@7" pad="37"/>
<connect gate="G$1" pin="NC@8" pad="38"/>
<connect gate="G$1" pin="NC@9" pad="71"/>
<connect gate="G$1" pin="R/!W" pad="23"/>
<connect gate="G$1" pin="READY" pad="19"/>
<connect gate="G$1" pin="TCK" pad="88"/>
<connect gate="G$1" pin="TDI" pad="86"/>
<connect gate="G$1" pin="TDO" pad="85"/>
<connect gate="G$1" pin="TMS" pad="89"/>
<connect gate="G$1" pin="TOUT0" pad="82"/>
<connect gate="G$1" pin="VSS@1" pad="3"/>
<connect gate="G$1" pin="VSS@10" pad="106"/>
<connect gate="G$1" pin="VSS@11" pad="111"/>
<connect gate="G$1" pin="VSS@12" pad="76"/>
<connect gate="G$1" pin="VSS@2" pad="14"/>
<connect gate="G$1" pin="VSS@3" pad="34"/>
<connect gate="G$1" pin="VSS@4" pad="40"/>
<connect gate="G$1" pin="VSS@5" pad="50"/>
<connect gate="G$1" pin="VSS@6" pad="57"/>
<connect gate="G$1" pin="VSS@7" pad="70"/>
<connect gate="G$1" pin="VSS@8" pad="93"/>
<connect gate="G$1" pin="VSS@9" pad="128"/>
<connect gate="G$1" pin="X1" pad="96"/>
<connect gate="G$1" pin="X2" pad="97"/>
<connect gate="G$1" pin="XF" pad="27"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TMS320VC5402PGE100"/>
<attribute name="OC_FARNELL" value="1214352"/>
<attribute name="OC_NEWARK" value="72K9586"/>
</technology>
</technologies>
</device>
<device name="GGU" package="PBGA144">
<connects>
<connect gate="G$1" pin="!BIO" pad="K3"/>
<connect gate="G$1" pin="!DS" pad="H1"/>
<connect gate="G$1" pin="!HAS" pad="F4"/>
<connect gate="G$1" pin="!HCS" pad="G2"/>
<connect gate="G$1" pin="!HDS1" pad="C7"/>
<connect gate="G$1" pin="!HDS2" pad="A6"/>
<connect gate="G$1" pin="!HINT!/OUT1" pad="M6"/>
<connect gate="G$1" pin="!HOLD" pad="K2"/>
<connect gate="G$1" pin="!HOLDA" pad="J4"/>
<connect gate="G$1" pin="!IACK" pad="N9"/>
<connect gate="G$1" pin="!IAQ" pad="K1"/>
<connect gate="G$1" pin="!INT0" pad="K9"/>
<connect gate="G$1" pin="!INT1" pad="N10"/>
<connect gate="G$1" pin="!INT2" pad="M10"/>
<connect gate="G$1" pin="!INT3" pad="L10"/>
<connect gate="G$1" pin="!IOSTRB" pad="J1"/>
<connect gate="G$1" pin="!IS" pad="H2"/>
<connect gate="G$1" pin="!MSC" pad="J2"/>
<connect gate="G$1" pin="!MSTRB" pad="H4"/>
<connect gate="G$1" pin="!NMI" pad="L9"/>
<connect gate="G$1" pin="!PS" pad="G4"/>
<connect gate="G$1" pin="!RS" pad="E12"/>
<connect gate="G$1" pin="!TRST" pad="H12"/>
<connect gate="G$1" pin="A0" pad="C6"/>
<connect gate="G$1" pin="A1" pad="D6"/>
<connect gate="G$1" pin="A10" pad="D4"/>
<connect gate="G$1" pin="A11" pad="D2"/>
<connect gate="G$1" pin="A12" pad="D1"/>
<connect gate="G$1" pin="A13" pad="E4"/>
<connect gate="G$1" pin="A14" pad="E3"/>
<connect gate="G$1" pin="A15" pad="E2"/>
<connect gate="G$1" pin="A16" pad="C12"/>
<connect gate="G$1" pin="A17" pad="B13"/>
<connect gate="G$1" pin="A18" pad="B12"/>
<connect gate="G$1" pin="A19" pad="A13"/>
<connect gate="G$1" pin="A2" pad="A5"/>
<connect gate="G$1" pin="A3" pad="B5"/>
<connect gate="G$1" pin="A4" pad="D5"/>
<connect gate="G$1" pin="A5" pad="A4"/>
<connect gate="G$1" pin="A6" pad="B4"/>
<connect gate="G$1" pin="A7" pad="C4"/>
<connect gate="G$1" pin="A8" pad="A3"/>
<connect gate="G$1" pin="A9" pad="B3"/>
<connect gate="G$1" pin="BCLKR0" pad="K4"/>
<connect gate="G$1" pin="BCLKR1" pad="L4"/>
<connect gate="G$1" pin="BCLKX0" pad="N5"/>
<connect gate="G$1" pin="BCLKX1" pad="K6"/>
<connect gate="G$1" pin="BDR0" pad="K5"/>
<connect gate="G$1" pin="BDR1" pad="M5"/>
<connect gate="G$1" pin="BDX0" pad="L8"/>
<connect gate="G$1" pin="BDX1" pad="K8"/>
<connect gate="G$1" pin="BFSR0" pad="M4"/>
<connect gate="G$1" pin="BFSR1" pad="N4"/>
<connect gate="G$1" pin="BFSX0" pad="M7"/>
<connect gate="G$1" pin="BFSX1" pad="N7"/>
<connect gate="G$1" pin="CLKMD1" pad="K10"/>
<connect gate="G$1" pin="CLKMD2" pad="K11"/>
<connect gate="G$1" pin="CLKMD3" pad="K12"/>
<connect gate="G$1" pin="CLKOUT" pad="F12"/>
<connect gate="G$1" pin="CVDD@1" pad="F1"/>
<connect gate="G$1" pin="CVDD@2" pad="G11"/>
<connect gate="G$1" pin="CVDD@3" pad="N6"/>
<connect gate="G$1" pin="CVDD@4" pad="N11"/>
<connect gate="G$1" pin="CVDD@5" pad="B7"/>
<connect gate="G$1" pin="CVDD@6" pad="C3"/>
<connect gate="G$1" pin="D0" pad="E11"/>
<connect gate="G$1" pin="D1" pad="E10"/>
<connect gate="G$1" pin="D10" pad="D9"/>
<connect gate="G$1" pin="D11" pad="C9"/>
<connect gate="G$1" pin="D12" pad="B9"/>
<connect gate="G$1" pin="D13" pad="D8"/>
<connect gate="G$1" pin="D14" pad="C8"/>
<connect gate="G$1" pin="D15" pad="B8"/>
<connect gate="G$1" pin="D2" pad="D13"/>
<connect gate="G$1" pin="D3" pad="D12"/>
<connect gate="G$1" pin="D4" pad="D11"/>
<connect gate="G$1" pin="D5" pad="C13"/>
<connect gate="G$1" pin="D6" pad="D10"/>
<connect gate="G$1" pin="D7" pad="C10"/>
<connect gate="G$1" pin="D8" pad="B10"/>
<connect gate="G$1" pin="D9" pad="A10"/>
<connect gate="G$1" pin="DVDD@0" pad="C1"/>
<connect gate="G$1" pin="DVDD@1" pad="L2"/>
<connect gate="G$1" pin="DVDD@2" pad="L12"/>
<connect gate="G$1" pin="DVDD@3" pad="K7"/>
<connect gate="G$1" pin="DVDD@4" pad="A11"/>
<connect gate="G$1" pin="DVDD@5" pad="B6"/>
<connect gate="G$1" pin="EMU0" pad="J12"/>
<connect gate="G$1" pin="EMU1" pad="J13"/>
<connect gate="G$1" pin="HBIL" pad="M9"/>
<connect gate="G$1" pin="HCNTL0" pad="M3"/>
<connect gate="G$1" pin="HCNTL1" pad="L5"/>
<connect gate="G$1" pin="HD0" pad="M8"/>
<connect gate="G$1" pin="HD1" pad="M11"/>
<connect gate="G$1" pin="HD2" pad="J10"/>
<connect gate="G$1" pin="HD3" pad="F11"/>
<connect gate="G$1" pin="HD4" pad="A9"/>
<connect gate="G$1" pin="HD5" pad="A8"/>
<connect gate="G$1" pin="HD6" pad="C5"/>
<connect gate="G$1" pin="HD7" pad="D3"/>
<connect gate="G$1" pin="HPIENA" pad="G10"/>
<connect gate="G$1" pin="HR/!W" pad="G1"/>
<connect gate="G$1" pin="HRDY" pad="L7"/>
<connect gate="G$1" pin="MP/!MC" pad="L1"/>
<connect gate="G$1" pin="NC@1" pad="A1"/>
<connect gate="G$1" pin="NC@10" pad="G13"/>
<connect gate="G$1" pin="NC@11" pad="N1"/>
<connect gate="G$1" pin="NC@12" pad="N2"/>
<connect gate="G$1" pin="NC@13" pad="N12"/>
<connect gate="G$1" pin="NC@14" pad="M12"/>
<connect gate="G$1" pin="NC@15" pad="A12"/>
<connect gate="G$1" pin="NC@16" pad="A7"/>
<connect gate="G$1" pin="NC@17" pad="A2"/>
<connect gate="G$1" pin="NC@18" pad="B2"/>
<connect gate="G$1" pin="NC@2" pad="B1"/>
<connect gate="G$1" pin="NC@3" pad="E1"/>
<connect gate="G$1" pin="NC@4" pad="F2"/>
<connect gate="G$1" pin="NC@5" pad="M1"/>
<connect gate="G$1" pin="NC@6" pad="M2"/>
<connect gate="G$1" pin="NC@7" pad="N13"/>
<connect gate="G$1" pin="NC@8" pad="M13"/>
<connect gate="G$1" pin="NC@9" pad="K13"/>
<connect gate="G$1" pin="R/!W" pad="H3"/>
<connect gate="G$1" pin="READY" pad="G3"/>
<connect gate="G$1" pin="TCK" pad="H13"/>
<connect gate="G$1" pin="TDI" pad="H11"/>
<connect gate="G$1" pin="TDO" pad="H10"/>
<connect gate="G$1" pin="TMS" pad="G12"/>
<connect gate="G$1" pin="TOUT0" pad="J11"/>
<connect gate="G$1" pin="VSS@1" pad="C2"/>
<connect gate="G$1" pin="VSS@10" pad="L11"/>
<connect gate="G$1" pin="VSS@11" pad="B11"/>
<connect gate="G$1" pin="VSS@12" pad="D7"/>
<connect gate="G$1" pin="VSS@2" pad="F3"/>
<connect gate="G$1" pin="VSS@3" pad="L3"/>
<connect gate="G$1" pin="VSS@4" pad="L13"/>
<connect gate="G$1" pin="VSS@5" pad="F13"/>
<connect gate="G$1" pin="VSS@6" pad="C11"/>
<connect gate="G$1" pin="VSS@7" pad="N3"/>
<connect gate="G$1" pin="VSS@8" pad="L6"/>
<connect gate="G$1" pin="VSS@9" pad="N8"/>
<connect gate="G$1" pin="X1" pad="F10"/>
<connect gate="G$1" pin="X2" pad="E13"/>
<connect gate="G$1" pin="XF" pad="J3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TMS320VC5402GGU100"/>
<attribute name="OC_FARNELL" value="1690105"/>
<attribute name="OC_NEWARK" value="76C9605"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC77*" prefix="IC">
<description>&lt;b&gt;MICROPOWER SUPPLY VOLTAGE SUPERVISORS&lt;/b&gt;&lt;p&gt;
Source: www.ti.com/.. slvs087l.pdf</description>
<gates>
<gate name="G$1" symbol="TLC77XX"/>
</gates>
<devices>
<device name="D" package="DIL08">
<connects>
<connect gate="G$1" pin="!RESET" pad="5"/>
<connect gate="G$1" pin="!RESIN" pad="2"/>
<connect gate="G$1" pin="CONTROL" pad="1"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="03">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7703QPE4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="24K5359"/>
</technology>
<technology name="05">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7705QP"/>
<attribute name="OC_FARNELL" value="8454671"/>
<attribute name="OC_NEWARK" value="76C7537"/>
</technology>
<technology name="25">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7725QP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="76C7546"/>
</technology>
<technology name="33">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7733QP"/>
<attribute name="OC_FARNELL" value="1411422"/>
<attribute name="OC_NEWARK" value="76C7553"/>
</technology>
</technologies>
</device>
<device name="PW" package="PW_R-PDSO-G08">
<connects>
<connect gate="G$1" pin="!RESET" pad="5"/>
<connect gate="G$1" pin="!RESIN" pad="2"/>
<connect gate="G$1" pin="CONTROL" pad="1"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TLC7701IPWR"/>
<attribute name="OC_FARNELL" value="1461368"/>
<attribute name="OC_NEWARK" value="76C7519"/>
</technology>
<technology name="03">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7703IPW"/>
<attribute name="OC_FARNELL" value="1411411"/>
<attribute name="OC_NEWARK" value="76C7527"/>
</technology>
<technology name="05">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7705QPW"/>
<attribute name="OC_FARNELL" value="1411414"/>
<attribute name="OC_NEWARK" value="95H4505"/>
</technology>
<technology name="25">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TLC7725IPWG4"/>
<attribute name="OC_FARNELL" value="1411418"/>
<attribute name="OC_NEWARK" value="18M3172"/>
</technology>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TLC7733QPWG4"/>
<attribute name="OC_FARNELL" value="1411423"/>
<attribute name="OC_NEWARK" value="54K1054"/>
</technology>
</technologies>
</device>
<device name="FK" package="PLCC20">
<connects>
<connect gate="G$1" pin="!RESET" pad="12"/>
<connect gate="G$1" pin="!RESIN" pad="5"/>
<connect gate="G$1" pin="CONTROL" pad="1"/>
<connect gate="G$1" pin="CT" pad="7"/>
<connect gate="G$1" pin="GND" pad="10"/>
<connect gate="G$1" pin="RESET" pad="15"/>
<connect gate="G$1" pin="SENSE" pad="17"/>
<connect gate="G$1" pin="VDD" pad="20"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="25">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="33">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="!RESET" pad="5"/>
<connect gate="G$1" pin="!RESIN" pad="2"/>
<connect gate="G$1" pin="CONTROL" pad="1"/>
<connect gate="G$1" pin="CT" pad="3"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RESET" pad="6"/>
<connect gate="G$1" pin="SENSE" pad="7"/>
<connect gate="G$1" pin="VDD" pad="8"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7701IP"/>
<attribute name="OC_FARNELL" value="1411405"/>
<attribute name="OC_NEWARK" value="76C7517"/>
</technology>
<technology name="03">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7703QP"/>
<attribute name="OC_FARNELL" value="1287644"/>
<attribute name="OC_NEWARK" value="76C7531"/>
</technology>
<technology name="05">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7705IP"/>
<attribute name="OC_FARNELL" value="1510448"/>
<attribute name="OC_NEWARK" value="35K1227"/>
</technology>
<technology name="25">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7725IP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="76C7541"/>
</technology>
<technology name="33">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7733QP"/>
<attribute name="OC_FARNELL" value="1411422"/>
<attribute name="OC_NEWARK" value="76C7553"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430F1*" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Family Members Include:&lt;br&gt;
- MSP430F133: 8KB+256B Flash Memory, 256B RAM&lt;br&gt;
- MSP430F135: 16KB+256B Flash Memory, 512B RAM&lt;br&gt;
- MSP430F147, MSP430F1471: 32KB+256B Flash Memory, 1KB RAM&lt;br&gt;
- MSP430F148, MSP430F1481: 48KB+256B Flash Memory, 2KB RAM&lt;br&gt;
- MSP430F149, MSP430F1491: 60KB+256B Flash Memory, 2KB RAM</description>
<gates>
<gate name="G$1" symbol="MSP430F149"/>
</gates>
<devices>
<device name="" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="!RTS!/NMI" pad="58"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="AVSS" pad="62"/>
<connect gate="G$1" pin="DVCC" pad="1"/>
<connect gate="G$1" pin="DVSS" pad="63"/>
<connect gate="G$1" pin="P1.0" pad="12"/>
<connect gate="G$1" pin="P1.1" pad="13"/>
<connect gate="G$1" pin="P1.2" pad="14"/>
<connect gate="G$1" pin="P1.3" pad="15"/>
<connect gate="G$1" pin="P1.4" pad="16"/>
<connect gate="G$1" pin="P1.5" pad="17"/>
<connect gate="G$1" pin="P1.6" pad="18"/>
<connect gate="G$1" pin="P1.7" pad="19"/>
<connect gate="G$1" pin="P2.0" pad="20"/>
<connect gate="G$1" pin="P2.1" pad="21"/>
<connect gate="G$1" pin="P2.2" pad="22"/>
<connect gate="G$1" pin="P2.3" pad="23"/>
<connect gate="G$1" pin="P2.4" pad="24"/>
<connect gate="G$1" pin="P2.5" pad="25"/>
<connect gate="G$1" pin="P2.6" pad="26"/>
<connect gate="G$1" pin="P2.7" pad="27"/>
<connect gate="G$1" pin="P3.0" pad="28"/>
<connect gate="G$1" pin="P3.1" pad="29"/>
<connect gate="G$1" pin="P3.2" pad="30"/>
<connect gate="G$1" pin="P3.3" pad="31"/>
<connect gate="G$1" pin="P3.4" pad="32"/>
<connect gate="G$1" pin="P3.5" pad="33"/>
<connect gate="G$1" pin="P3.6" pad="34"/>
<connect gate="G$1" pin="P3.7" pad="35"/>
<connect gate="G$1" pin="P4.0" pad="36"/>
<connect gate="G$1" pin="P4.1" pad="37"/>
<connect gate="G$1" pin="P4.2" pad="38"/>
<connect gate="G$1" pin="P4.3" pad="39"/>
<connect gate="G$1" pin="P4.4" pad="40"/>
<connect gate="G$1" pin="P4.5" pad="41"/>
<connect gate="G$1" pin="P4.6" pad="42"/>
<connect gate="G$1" pin="P4.7" pad="43"/>
<connect gate="G$1" pin="P5.0" pad="44"/>
<connect gate="G$1" pin="P5.1" pad="45"/>
<connect gate="G$1" pin="P5.2" pad="46"/>
<connect gate="G$1" pin="P5.3" pad="47"/>
<connect gate="G$1" pin="P5.4" pad="48"/>
<connect gate="G$1" pin="P5.5" pad="49"/>
<connect gate="G$1" pin="P5.6" pad="50"/>
<connect gate="G$1" pin="P5.7" pad="51"/>
<connect gate="G$1" pin="P6.0" pad="59"/>
<connect gate="G$1" pin="P6.1" pad="60"/>
<connect gate="G$1" pin="P6.2" pad="61"/>
<connect gate="G$1" pin="P6.3" pad="2"/>
<connect gate="G$1" pin="P6.4" pad="3"/>
<connect gate="G$1" pin="P6.5" pad="4"/>
<connect gate="G$1" pin="P6.6" pad="5"/>
<connect gate="G$1" pin="P6.7" pad="6"/>
<connect gate="G$1" pin="TCK" pad="57"/>
<connect gate="G$1" pin="TDI" pad="55"/>
<connect gate="G$1" pin="TDO/TDI" pad="54"/>
<connect gate="G$1" pin="TMS" pad="56"/>
<connect gate="G$1" pin="VEREF+" pad="10"/>
<connect gate="G$1" pin="VREF+" pad="7"/>
<connect gate="G$1" pin="VREF-/VEREF-" pad="11"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT/TCLK" pad="9"/>
<connect gate="G$1" pin="XT2IN" pad="53"/>
<connect gate="G$1" pin="XT2OUT" pad="52"/>
</connects>
<technologies>
<technology name="33">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="MSP430F133IPM"/>
<attribute name="OC_FARNELL" value="1471268"/>
<attribute name="OC_NEWARK" value="75C4034"/>
</technology>
<technology name="35">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="MSP430F135IPM"/>
<attribute name="OC_FARNELL" value="1106050"/>
<attribute name="OC_NEWARK" value="75C4036"/>
</technology>
<technology name="47">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F1471IPM"/>
<attribute name="OC_FARNELL" value="1649389"/>
<attribute name="OC_NEWARK" value="95M6746"/>
</technology>
<technology name="471">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F1471IRTDT"/>
<attribute name="OC_FARNELL" value="1537163"/>
<attribute name="OC_NEWARK" value="95M6747"/>
</technology>
<technology name="48">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F1481IPM"/>
<attribute name="OC_FARNELL" value="1649391"/>
<attribute name="OC_NEWARK" value="95M6750"/>
</technology>
<technology name="481">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F1481IPM"/>
<attribute name="OC_FARNELL" value="1649391"/>
<attribute name="OC_NEWARK" value="95M6750"/>
</technology>
<technology name="49">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F1491IRTDT"/>
<attribute name="OC_FARNELL" value="1537170"/>
<attribute name="OC_NEWARK" value="95M6752"/>
</technology>
<technology name="491">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="MSP430F1491IPM"/>
<attribute name="OC_FARNELL" value="1537169"/>
<attribute name="OC_NEWARK" value="34K8186"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="THS4211" prefix="IC">
<description>&lt;b&gt;LOW-DISTORTION, HIGH-SPEED, VOLTAGE FEEDBACK AMPLIFIER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ths4211.pdf</description>
<gates>
<gate name="G$1" symbol="OPAMP+-"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="S-PDSO-G08">
<connects>
<connect gate="G$1" pin="+IN" pad="3"/>
<connect gate="G$1" pin="-IN" pad="2"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="V+" pad="7"/>
<connect gate="G$1" pin="V-" pad="4"/>
<connect gate="TH" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="THS4211DGK"/>
<attribute name="OC_FARNELL" value="8453306"/>
<attribute name="OC_NEWARK" value="95H4489"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM3006" prefix="IC">
<description>&lt;b&gt;16-Bit, Single-Ended Analog Input/Output Stereo Audio Codec&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm3006.pdf</description>
<gates>
<gate name="G$1" symbol="PCM3006"/>
</gates>
<devices>
<device name="" package="R-PSOP-G24">
<connects>
<connect gate="G$1" pin="!PDAD" pad="7"/>
<connect gate="G$1" pin="!PDDA" pad="8"/>
<connect gate="G$1" pin="BCKIN" pad="11"/>
<connect gate="G$1" pin="DEM0" pad="18"/>
<connect gate="G$1" pin="DEM1" pad="17"/>
<connect gate="G$1" pin="DIN" pad="15"/>
<connect gate="G$1" pin="DOUT" pad="12"/>
<connect gate="G$1" pin="GND@D" pad="13"/>
<connect gate="G$1" pin="GNDA" pad="22"/>
<connect gate="G$1" pin="LRCIN" pad="10"/>
<connect gate="G$1" pin="SYSCLOCK" pad="9"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC1@1" pad="2"/>
<connect gate="G$1" pin="VCC2" pad="24"/>
<connect gate="G$1" pin="VCOM" pad="21"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VINL" pad="6"/>
<connect gate="G$1" pin="VINR" pad="3"/>
<connect gate="G$1" pin="VOUTL" pad="19"/>
<connect gate="G$1" pin="VOUTR" pad="20"/>
<connect gate="G$1" pin="VREF1" pad="4"/>
<connect gate="G$1" pin="VREF2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM3006T"/>
<attribute name="OC_FARNELL" value="1510088"/>
<attribute name="OC_NEWARK" value="75C5392"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS75003" prefix="IC">
<description>&lt;b&gt;Triple-Supply Power Management IC&lt;/b&gt; for Powering FPGAs and DSPs&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps75003.pdf</description>
<gates>
<gate name="G$1" symbol="TPS75003"/>
</gates>
<devices>
<device name="" package="R-PQFP-N20">
<connects>
<connect gate="G$1" pin="AGND" pad="18"/>
<connect gate="G$1" pin="DGND" pad="6"/>
<connect gate="G$1" pin="DGND@1" pad="15"/>
<connect gate="G$1" pin="DGND@2" pad="E@1"/>
<connect gate="G$1" pin="DGND@3" pad="E@2"/>
<connect gate="G$1" pin="DGND@4" pad="E@3"/>
<connect gate="G$1" pin="DGND@5" pad="E@4"/>
<connect gate="G$1" pin="EN1" pad="17"/>
<connect gate="G$1" pin="EN2" pad="4"/>
<connect gate="G$1" pin="EN3" pad="3"/>
<connect gate="G$1" pin="FB1" pad="11"/>
<connect gate="G$1" pin="FB2" pad="10"/>
<connect gate="G$1" pin="FB3" pad="2"/>
<connect gate="G$1" pin="IN1" pad="13"/>
<connect gate="G$1" pin="IN2" pad="8"/>
<connect gate="G$1" pin="IN3" pad="20"/>
<connect gate="G$1" pin="IS1" pad="12"/>
<connect gate="G$1" pin="IS2" pad="9"/>
<connect gate="G$1" pin="OUT3" pad="1"/>
<connect gate="G$1" pin="SS1" pad="16"/>
<connect gate="G$1" pin="SS2" pad="5"/>
<connect gate="G$1" pin="SS3" pad="19"/>
<connect gate="G$1" pin="SW1" pad="14"/>
<connect gate="G$1" pin="SW2" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS75003RHLT"/>
<attribute name="OC_FARNELL" value="9969187"/>
<attribute name="OC_NEWARK" value="93K0913"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ2412*" prefix="IC">
<description>&lt;b&gt;SINGLE-CHIP SWITCHMODE, LI-ION AND LI-POLYMER CHARGE-MANAGEMENT&lt;/b&gt;&lt;p&gt;
WITH ENHANCED EMI PERFORMANCE(bqSWITCHER TM)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/bq24120.pdf</description>
<gates>
<gate name="G$1" symbol="BQ24120"/>
</gates>
<devices>
<device name="" package="R-PQFP-N20">
<connects>
<connect gate="G$1" pin="!CE" pad="16"/>
<connect gate="G$1" pin="!PG" pad="5"/>
<connect gate="G$1" pin="BAT" pad="14"/>
<connect gate="G$1" pin="CELLS" pad="13"/>
<connect gate="G$1" pin="EXP@1" pad="E@1"/>
<connect gate="G$1" pin="EXP@2" pad="E@2"/>
<connect gate="G$1" pin="EXP@3" pad="E@3"/>
<connect gate="G$1" pin="EXP@4" pad="E@4"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="4"/>
<connect gate="G$1" pin="ISET1" pad="8"/>
<connect gate="G$1" pin="ISET2" pad="9"/>
<connect gate="G$1" pin="OUT1" pad="1"/>
<connect gate="G$1" pin="OUT2" pad="20"/>
<connect gate="G$1" pin="PGND@1" pad="17"/>
<connect gate="G$1" pin="PGND@2" pad="18"/>
<connect gate="G$1" pin="SNS" pad="15"/>
<connect gate="G$1" pin="STAT1" pad="2"/>
<connect gate="G$1" pin="STAT2" pad="19"/>
<connect gate="G$1" pin="TS" pad="12"/>
<connect gate="G$1" pin="TTC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VSS" pad="10"/>
<connect gate="G$1" pin="VTSB" pad="11"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ24120RHLTG4"/>
<attribute name="OC_FARNELL" value="1230453"/>
<attribute name="OC_NEWARK" value="12M9386"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ24123RHLT"/>
<attribute name="OC_FARNELL" value="1407131"/>
<attribute name="OC_NEWARK" value="84K0851"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL16C754B" prefix="IC">
<description>&lt;b&gt;QUAD UART WITH 64-BYTE FIFO&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tl16c754b.pdf</description>
<gates>
<gate name="G$1" symbol="TL16C754B"/>
</gates>
<devices>
<device name="" package="PLCC68S">
<connects>
<connect gate="G$1" pin="!CDA" pad="9"/>
<connect gate="G$1" pin="!CDB" pad="27"/>
<connect gate="G$1" pin="!CDC" pad="43"/>
<connect gate="G$1" pin="!CDD" pad="61"/>
<connect gate="G$1" pin="!CSA" pad="16"/>
<connect gate="G$1" pin="!CSB" pad="20"/>
<connect gate="G$1" pin="!CSC" pad="50"/>
<connect gate="G$1" pin="!CSD" pad="54"/>
<connect gate="G$1" pin="!CTSA" pad="11"/>
<connect gate="G$1" pin="!CTSB" pad="25"/>
<connect gate="G$1" pin="!CTSC" pad="45"/>
<connect gate="G$1" pin="!CTSD" pad="59"/>
<connect gate="G$1" pin="!DSRA" pad="10"/>
<connect gate="G$1" pin="!DSRB" pad="26"/>
<connect gate="G$1" pin="!DSRC" pad="44"/>
<connect gate="G$1" pin="!DSRD" pad="60"/>
<connect gate="G$1" pin="!DTRA" pad="12"/>
<connect gate="G$1" pin="!DTRB" pad="24"/>
<connect gate="G$1" pin="!DTRC" pad="46"/>
<connect gate="G$1" pin="!DTRD" pad="58"/>
<connect gate="G$1" pin="!IOR" pad="52"/>
<connect gate="G$1" pin="!IOW" pad="18"/>
<connect gate="G$1" pin="!RIA" pad="8"/>
<connect gate="G$1" pin="!RIB" pad="28"/>
<connect gate="G$1" pin="!RIC" pad="42"/>
<connect gate="G$1" pin="!RID" pad="62"/>
<connect gate="G$1" pin="!RTSA" pad="14"/>
<connect gate="G$1" pin="!RTSB" pad="22"/>
<connect gate="G$1" pin="!RTSC" pad="48"/>
<connect gate="G$1" pin="!RTSD" pad="56"/>
<connect gate="G$1" pin="!RXRDY" pad="38"/>
<connect gate="G$1" pin="!TXRDY" pad="39"/>
<connect gate="G$1" pin="A0" pad="34"/>
<connect gate="G$1" pin="A1" pad="33"/>
<connect gate="G$1" pin="A2" pad="32"/>
<connect gate="G$1" pin="CLKSEL" pad="30"/>
<connect gate="G$1" pin="D0" pad="66"/>
<connect gate="G$1" pin="D1" pad="67"/>
<connect gate="G$1" pin="D2" pad="68"/>
<connect gate="G$1" pin="D3" pad="1"/>
<connect gate="G$1" pin="D4" pad="2"/>
<connect gate="G$1" pin="D5" pad="3"/>
<connect gate="G$1" pin="D6" pad="4"/>
<connect gate="G$1" pin="D7" pad="5"/>
<connect gate="G$1" pin="GND" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="23"/>
<connect gate="G$1" pin="GND@2" pad="40"/>
<connect gate="G$1" pin="GND@3" pad="57"/>
<connect gate="G$1" pin="INTA" pad="15"/>
<connect gate="G$1" pin="INTB" pad="21"/>
<connect gate="G$1" pin="INTC" pad="49"/>
<connect gate="G$1" pin="INTD" pad="55"/>
<connect gate="G$1" pin="INTESEL" pad="65"/>
<connect gate="G$1" pin="NC" pad="31"/>
<connect gate="G$1" pin="RESET" pad="37"/>
<connect gate="G$1" pin="RXA" pad="7"/>
<connect gate="G$1" pin="RXB" pad="29"/>
<connect gate="G$1" pin="RXC" pad="41"/>
<connect gate="G$1" pin="RXD" pad="63"/>
<connect gate="G$1" pin="TXA" pad="17"/>
<connect gate="G$1" pin="TXB" pad="19"/>
<connect gate="G$1" pin="TXC" pad="51"/>
<connect gate="G$1" pin="TXD" pad="53"/>
<connect gate="G$1" pin="VCC" pad="13"/>
<connect gate="G$1" pin="VCC@1" pad="47"/>
<connect gate="G$1" pin="VCC@2" pad="64"/>
<connect gate="G$1" pin="XTAL1" pad="35"/>
<connect gate="G$1" pin="XTAL2" pad="36"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TL16C754BFN"/>
<attribute name="OC_FARNELL" value="1659627"/>
<attribute name="OC_NEWARK" value="12P7902"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="75ALS176" prefix="IC">
<description>&lt;b&gt;DIFFERENTIAL BUS TRANSCEIVERS&lt;/b&gt;&lt;p&gt;
TIA/EIA-422-B,  TIA/EIA-422-B + TIA/EIA-422-B TIA/EIA-422-B&lt;br&gt;
Operate at Data Rates up to 35 Mbaud&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn65als176.pdf</description>
<gates>
<gate name="-1" symbol="75ALS176"/>
<gate name="P" symbol="VCCGND"/>
</gates>
<devices>
<device name="D" package="SO-08">
<connects>
<connect gate="-1" pin="!RE" pad="2"/>
<connect gate="-1" pin="A" pad="6"/>
<connect gate="-1" pin="B" pad="7"/>
<connect gate="-1" pin="D" pad="4"/>
<connect gate="-1" pin="DE" pad="3"/>
<connect gate="-1" pin="R" pad="1"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="SN75ALS176D"/>
<attribute name="OC_FARNELL" value="9593020"/>
<attribute name="OC_NEWARK" value="08F8011"/>
</technology>
<technology name="A">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="SN75ALS176AD"/>
<attribute name="OC_FARNELL" value="1410742"/>
<attribute name="OC_NEWARK" value="76C5099"/>
</technology>
<technology name="B">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="SN75ALS176BD"/>
<attribute name="OC_FARNELL" value="9593012"/>
<attribute name="OC_NEWARK" value="35K0833"/>
</technology>
</technologies>
</device>
<device name="P" package="DIL08">
<connects>
<connect gate="-1" pin="!RE" pad="2"/>
<connect gate="-1" pin="A" pad="6"/>
<connect gate="-1" pin="B" pad="7"/>
<connect gate="-1" pin="D" pad="4"/>
<connect gate="-1" pin="DE" pad="3"/>
<connect gate="-1" pin="R" pad="1"/>
<connect gate="P" pin="GND" pad="5"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="SN75ALS176P"/>
<attribute name="OC_FARNELL" value="1103021"/>
<attribute name="OC_NEWARK" value="60K6915"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6107*" prefix="IC">
<description>&lt;b&gt;90% EFFICIENT SYNCHRONOUS BOOST CONVERTER WITH 600-mA SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps61070.pdf</description>
<gates>
<gate name="G$1" symbol="TPS61070"/>
</gates>
<devices>
<device name="DDC" package="TSOT23-6_DDC">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SW" pad="1"/>
<connect gate="G$1" pin="VBAT" pad="6"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS61070DDCR"/>
<attribute name="OC_FARNELL" value="1461062"/>
<attribute name="OC_NEWARK" value="64M3125"/>
</technology>
<technology name="1">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TPS61071DDCR"/>
<attribute name="OC_FARNELL" value="1412515"/>
<attribute name="OC_NEWARK" value="21J9232"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS61072DDCR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="30M1829"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS61073DDCRG4"/>
<attribute name="OC_FARNELL" value="1755459"/>
<attribute name="OC_NEWARK" value="52M6122"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DDC232" prefix="IC">
<description>&lt;b&gt;32-Channel, Current-Input Analog-to-Digital Converter&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ddc232.pdf</description>
<gates>
<gate name="G$1" symbol="DDC232"/>
</gates>
<devices>
<device name="" package="PBGA-N64">
<connects>
<connect gate="G$1" pin="!DVALID" pad="H7"/>
<connect gate="G$1" pin="!RESET" pad="C7"/>
<connect gate="G$1" pin="AGND" pad="A5"/>
<connect gate="G$1" pin="AGND@1" pad="B5"/>
<connect gate="G$1" pin="AGND@2" pad="C5"/>
<connect gate="G$1" pin="AGND@3" pad="D5"/>
<connect gate="G$1" pin="AGND@4" pad="D6"/>
<connect gate="G$1" pin="AGND@5" pad="E5"/>
<connect gate="G$1" pin="AGND@6" pad="F5"/>
<connect gate="G$1" pin="AGND@7" pad="G5"/>
<connect gate="G$1" pin="AGND@8" pad="H6"/>
<connect gate="G$1" pin="AVDD" pad="E6"/>
<connect gate="G$1" pin="AVDD@1" pad="E7"/>
<connect gate="G$1" pin="AVDD@2" pad="F6"/>
<connect gate="G$1" pin="AVDD@3" pad="G6"/>
<connect gate="G$1" pin="CLK" pad="F8"/>
<connect gate="G$1" pin="CLK_CFG" pad="F7"/>
<connect gate="G$1" pin="CONV" pad="A8"/>
<connect gate="G$1" pin="DCLK" pad="H8"/>
<connect gate="G$1" pin="DGND" pad="A7"/>
<connect gate="G$1" pin="DGND@1" pad="C6"/>
<connect gate="G$1" pin="DGND@2" pad="C8"/>
<connect gate="G$1" pin="DGND@3" pad="D7"/>
<connect gate="G$1" pin="DGND@4" pad="G8"/>
<connect gate="G$1" pin="DIN" pad="B8"/>
<connect gate="G$1" pin="DIN_CFG" pad="G7"/>
<connect gate="G$1" pin="DOUT" pad="D8"/>
<connect gate="G$1" pin="DVDD" pad="B7"/>
<connect gate="G$1" pin="IN1" pad="H4"/>
<connect gate="G$1" pin="IN10" pad="C2"/>
<connect gate="G$1" pin="IN11" pad="B2"/>
<connect gate="G$1" pin="IN12" pad="A2"/>
<connect gate="G$1" pin="IN13" pad="D4"/>
<connect gate="G$1" pin="IN14" pad="C4"/>
<connect gate="G$1" pin="IN15" pad="B4"/>
<connect gate="G$1" pin="IN16" pad="A4"/>
<connect gate="G$1" pin="IN17" pad="H3"/>
<connect gate="G$1" pin="IN18" pad="G3"/>
<connect gate="G$1" pin="IN19" pad="F3"/>
<connect gate="G$1" pin="IN2" pad="G4"/>
<connect gate="G$1" pin="IN20" pad="E3"/>
<connect gate="G$1" pin="IN21" pad="H1"/>
<connect gate="G$1" pin="IN22" pad="G1"/>
<connect gate="G$1" pin="IN23" pad="F1"/>
<connect gate="G$1" pin="IN24" pad="E1"/>
<connect gate="G$1" pin="IN25" pad="D1"/>
<connect gate="G$1" pin="IN26" pad="C1"/>
<connect gate="G$1" pin="IN27" pad="B1"/>
<connect gate="G$1" pin="IN28" pad="A1"/>
<connect gate="G$1" pin="IN29" pad="D3"/>
<connect gate="G$1" pin="IN3" pad="F4"/>
<connect gate="G$1" pin="IN30" pad="C3"/>
<connect gate="G$1" pin="IN31" pad="B3"/>
<connect gate="G$1" pin="IN32" pad="A3"/>
<connect gate="G$1" pin="IN4" pad="E4"/>
<connect gate="G$1" pin="IN5" pad="H2"/>
<connect gate="G$1" pin="IN6" pad="G2"/>
<connect gate="G$1" pin="IN7" pad="F2"/>
<connect gate="G$1" pin="IN8" pad="E2"/>
<connect gate="G$1" pin="IN9" pad="D2"/>
<connect gate="G$1" pin="QGND" pad="H5"/>
<connect gate="G$1" pin="VREF" pad="A6"/>
<connect gate="G$1" pin="VREF@1" pad="B6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DDC232CGXGR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M7216"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6120*" prefix="IC">
<description>&lt;b&gt;LOW INPUT VOLTAGE SYNCHRONOUS BOOST CONVERTER WITH 1.3-A SWITCHES&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps61200.pdf</description>
<gates>
<gate name="G$1" symbol="TPS61200"/>
</gates>
<devices>
<device name="" package="S-PDSO-N10">
<connects>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="FB" pad="10"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="L" pad="3"/>
<connect gate="G$1" pin="PGND" pad="4"/>
<connect gate="G$1" pin="PP" pad="PP"/>
<connect gate="G$1" pin="PP@1" pad="PP@1"/>
<connect gate="G$1" pin="PP@2" pad="PP@2"/>
<connect gate="G$1" pin="PS" pad="8"/>
<connect gate="G$1" pin="UVLO" pad="7"/>
<connect gate="G$1" pin="VAUX" pad="1"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS61200DRCT"/>
<attribute name="OC_FARNELL" value="1471238"/>
<attribute name="OC_NEWARK" value="37M0066"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS61201DRCT"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M0068"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS61202DRCR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37M0069"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430FG4618" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 19&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/docs/prod/folders/print/msp430fg4618.html</description>
<gates>
<gate name="G$1" symbol="MSP430FG4618"/>
</gates>
<devices>
<device name="PZ" package="TQFP100">
<connects>
<connect gate="G$1" pin="AVCC" pad="100"/>
<connect gate="G$1" pin="AVSS" pad="98"/>
<connect gate="G$1" pin="COM0" pad="52"/>
<connect gate="G$1" pin="DVCC1" pad="1"/>
<connect gate="G$1" pin="DVCC2" pad="60"/>
<connect gate="G$1" pin="DVSS1" pad="99"/>
<connect gate="G$1" pin="DVSS2" pad="61"/>
<connect gate="G$1" pin="LCDCAP/R33" pad="59"/>
<connect gate="G$1" pin="P10_0/S9" pad="21"/>
<connect gate="G$1" pin="P10_1/S8" pad="20"/>
<connect gate="G$1" pin="P10_2/S7" pad="19"/>
<connect gate="G$1" pin="P10_3/S6" pad="18"/>
<connect gate="G$1" pin="P10_4/S5" pad="17"/>
<connect gate="G$1" pin="P10_5/S4" pad="16"/>
<connect gate="G$1" pin="P10_6/S3/A15" pad="15"/>
<connect gate="G$1" pin="P10_7/S2/A14/OA2I1" pad="14"/>
<connect gate="G$1" pin="P1_0/TA0" pad="87"/>
<connect gate="G$1" pin="P1_1/TA0/MCLK" pad="86"/>
<connect gate="G$1" pin="P1_2/TA1" pad="85"/>
<connect gate="G$1" pin="P1_3/TBOUTH/SVSOUT" pad="84"/>
<connect gate="G$1" pin="P1_4/TBCLK/SMCLK" pad="83"/>
<connect gate="G$1" pin="P1_5/TACLK/ACLK" pad="82"/>
<connect gate="G$1" pin="P1_6/CA0" pad="81"/>
<connect gate="G$1" pin="P1_7/CA1" pad="80"/>
<connect gate="G$1" pin="P2_0/TA2" pad="79"/>
<connect gate="G$1" pin="P2_1/TB0" pad="78"/>
<connect gate="G$1" pin="P2_2/TB1" pad="77"/>
<connect gate="G$1" pin="P2_3/TB2" pad="76"/>
<connect gate="G$1" pin="P2_4/UCA0TXD" pad="75"/>
<connect gate="G$1" pin="P2_5/UCA0RXD" pad="74"/>
<connect gate="G$1" pin="P2_6/CAOUT" pad="73"/>
<connect gate="G$1" pin="P2_7/ADC12CLK/DMAE0" pad="72"/>
<connect gate="G$1" pin="P3_0/UCB0STE" pad="71"/>
<connect gate="G$1" pin="P3_1/UCB0SIMO/UCB0SDA" pad="70"/>
<connect gate="G$1" pin="P3_2/UCB0SOMI/UCB0SCL" pad="69"/>
<connect gate="G$1" pin="P3_3/UCB0CLK" pad="68"/>
<connect gate="G$1" pin="P3_4/TB3" pad="67"/>
<connect gate="G$1" pin="P3_5/TB4" pad="66"/>
<connect gate="G$1" pin="P3_6/TB5" pad="65"/>
<connect gate="G$1" pin="P3_7/TB6" pad="64"/>
<connect gate="G$1" pin="P4_0/UTXD1" pad="63"/>
<connect gate="G$1" pin="P4_1/URXD1" pad="62"/>
<connect gate="G$1" pin="P4_2/STE1/S39" pad="51"/>
<connect gate="G$1" pin="P4_3/SIMO1/S38" pad="50"/>
<connect gate="G$1" pin="P4_4/SOMI1/S37" pad="49"/>
<connect gate="G$1" pin="P4_5/UCLK1/S36" pad="48"/>
<connect gate="G$1" pin="P4_6/UCA0TXD/S35" pad="47"/>
<connect gate="G$1" pin="P4_7/UCA0RXD/S34" pad="46"/>
<connect gate="G$1" pin="P5_0/S1/A13/OA1I1" pad="13"/>
<connect gate="G$1" pin="P5_1/S0/A12/DAC1" pad="12"/>
<connect gate="G$1" pin="P5_2/COM1" pad="53"/>
<connect gate="G$1" pin="P5_3/COM2" pad="54"/>
<connect gate="G$1" pin="P5_4/COM3" pad="55"/>
<connect gate="G$1" pin="P5_5/R03" pad="56"/>
<connect gate="G$1" pin="P5_6/LCDREF/R13" pad="57"/>
<connect gate="G$1" pin="P5_7/R23" pad="58"/>
<connect gate="G$1" pin="P6_0/A0/OA0I0" pad="95"/>
<connect gate="G$1" pin="P6_1/A1/OA0O" pad="96"/>
<connect gate="G$1" pin="P6_2/A2/OA0I1" pad="97"/>
<connect gate="G$1" pin="P6_3/A3/OA1O" pad="2"/>
<connect gate="G$1" pin="P6_4/A4/OA1I0" pad="3"/>
<connect gate="G$1" pin="P6_5/A5/OA2O" pad="4"/>
<connect gate="G$1" pin="P6_6/A6/DAC0/OA2I0" pad="5"/>
<connect gate="G$1" pin="P6_7/A7/DAC1/SVSIN" pad="6"/>
<connect gate="G$1" pin="P7_0/UCA0STE/S33" pad="45"/>
<connect gate="G$1" pin="P7_1/UCA0SIMO/S32" pad="44"/>
<connect gate="G$1" pin="P7_2/UCA0SOMI/S31" pad="43"/>
<connect gate="G$1" pin="P7_3/UCA0CLK/S30" pad="42"/>
<connect gate="G$1" pin="P7_4/S29" pad="41"/>
<connect gate="G$1" pin="P7_5/S28" pad="40"/>
<connect gate="G$1" pin="P7_6/S27" pad="39"/>
<connect gate="G$1" pin="P7_7/S26" pad="38"/>
<connect gate="G$1" pin="P8_0/S25" pad="37"/>
<connect gate="G$1" pin="P8_1/S24" pad="36"/>
<connect gate="G$1" pin="P8_2/S23" pad="35"/>
<connect gate="G$1" pin="P8_3/S22" pad="34"/>
<connect gate="G$1" pin="P8_4/S21" pad="33"/>
<connect gate="G$1" pin="P8_5/S20" pad="32"/>
<connect gate="G$1" pin="P8_6/S19" pad="31"/>
<connect gate="G$1" pin="P8_7/S18" pad="30"/>
<connect gate="G$1" pin="P9_0/S17" pad="29"/>
<connect gate="G$1" pin="P9_1/S16" pad="28"/>
<connect gate="G$1" pin="P9_2/S15" pad="27"/>
<connect gate="G$1" pin="P9_3/S14" pad="26"/>
<connect gate="G$1" pin="P9_4/S13" pad="25"/>
<connect gate="G$1" pin="P9_5/S12" pad="24"/>
<connect gate="G$1" pin="P9_6/S11" pad="23"/>
<connect gate="G$1" pin="P9_7/S10" pad="22"/>
<connect gate="G$1" pin="RST/NMI" pad="94"/>
<connect gate="G$1" pin="TCK" pad="93"/>
<connect gate="G$1" pin="TDI/TCLK" pad="91"/>
<connect gate="G$1" pin="TDO/TDI" pad="90"/>
<connect gate="G$1" pin="TMS" pad="92"/>
<connect gate="G$1" pin="VEREF+/DAC0" pad="10"/>
<connect gate="G$1" pin="VREF+" pad="7"/>
<connect gate="G$1" pin="VREF--/VEREF--" pad="11"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT" pad="9"/>
<connect gate="G$1" pin="XT2IN" pad="89"/>
<connect gate="G$1" pin="XT2OUT" pad="88"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430FG4618IPZ"/>
<attribute name="OC_FARNELL" value="1470488"/>
<attribute name="OC_NEWARK" value="22M1151"/>
</technology>
</technologies>
</device>
<device name="ZQW" package="S-PBGA-N113">
<connects>
<connect gate="G$1" pin="AVCC" pad="A2"/>
<connect gate="G$1" pin="AVSS" pad="A3"/>
<connect gate="G$1" pin="COM0" pad="L10"/>
<connect gate="G$1" pin="DVCC1" pad="A1"/>
<connect gate="G$1" pin="DVCC2" pad="H12"/>
<connect gate="G$1" pin="DVSS1" pad="B3"/>
<connect gate="G$1" pin="DVSS2" pad="G12"/>
<connect gate="G$1" pin="LCDCAP/R33" pad="H11"/>
<connect gate="G$1" pin="P10_0/S9" pad="J1"/>
<connect gate="G$1" pin="P10_1/S8" pad="F5"/>
<connect gate="G$1" pin="P10_2/S7" pad="H2"/>
<connect gate="G$1" pin="P10_3/S6" pad="H1"/>
<connect gate="G$1" pin="P10_4/S5" pad="F4"/>
<connect gate="G$1" pin="P10_5/S4" pad="G2"/>
<connect gate="G$1" pin="P10_6/S3/A15" pad="G1"/>
<connect gate="G$1" pin="P10_7/S2/A14/OA2I1" pad="E5"/>
<connect gate="G$1" pin="P1_0/TA0" pad="A7"/>
<connect gate="G$1" pin="P1_1/TA0/MCLK" pad="E7"/>
<connect gate="G$1" pin="P1_2/TA1" pad="D7"/>
<connect gate="G$1" pin="P1_3/TBOUTH/SVSOUT" pad="A8"/>
<connect gate="G$1" pin="P1_4/TBCLK/SMCLK" pad="B8"/>
<connect gate="G$1" pin="P1_5/TACLK/ACLK" pad="B9"/>
<connect gate="G$1" pin="P1_6/CA0" pad="A9"/>
<connect gate="G$1" pin="P1_7/CA1" pad="B10"/>
<connect gate="G$1" pin="P2_0/TA2" pad="A10"/>
<connect gate="G$1" pin="P2_1/TB0" pad="D8"/>
<connect gate="G$1" pin="P2_2/TB1" pad="E8"/>
<connect gate="G$1" pin="P2_3/TB2" pad="A11"/>
<connect gate="G$1" pin="P2_4/UCA0TXD" pad="B12"/>
<connect gate="G$1" pin="P2_5/UCA0RXD" pad="C11"/>
<connect gate="G$1" pin="P2_6/CAOUT" pad="C12"/>
<connect gate="G$1" pin="P2_7/ADC12CLK/DMAE0" pad="E9"/>
<connect gate="G$1" pin="P3_0/UCB0STE" pad="D11"/>
<connect gate="G$1" pin="P3_1/UCB0SIMO/UCB0SDA" pad="D12"/>
<connect gate="G$1" pin="P3_2/UCB0SOMI/UCB0SCL" pad="F9"/>
<connect gate="G$1" pin="P3_3/UCB0CLK" pad="E11"/>
<connect gate="G$1" pin="P3_4/TB3" pad="E12"/>
<connect gate="G$1" pin="P3_5/TB4" pad="G9"/>
<connect gate="G$1" pin="P3_6/TB5" pad="F11"/>
<connect gate="G$1" pin="P3_7/TB6" pad="F12"/>
<connect gate="G$1" pin="P4_0/UTXD1" pad="H9"/>
<connect gate="G$1" pin="P4_1/URXD1" pad="G11"/>
<connect gate="G$1" pin="P4_2/STE1/S39" pad="M11"/>
<connect gate="G$1" pin="P4_3/SIMO1/S38" pad="M10"/>
<connect gate="G$1" pin="P4_4/SOMI1/S37" pad="H7"/>
<connect gate="G$1" pin="P4_5/UCLK1/S36" pad="L9"/>
<connect gate="G$1" pin="P4_6/UCA0TXD/S35" pad="M9"/>
<connect gate="G$1" pin="P4_7/UCA0RXD/S34" pad="J7"/>
<connect gate="G$1" pin="P5_0/S1/A13/OA1I1" pad="F2"/>
<connect gate="G$1" pin="P5_1/S0/A12/DAC1" pad="F1"/>
<connect gate="G$1" pin="P5_2/COM1" pad="L12"/>
<connect gate="G$1" pin="P5_3/COM2" pad="J8"/>
<connect gate="G$1" pin="P5_4/COM3" pad="K12"/>
<connect gate="G$1" pin="P5_5/R03" pad="K11"/>
<connect gate="G$1" pin="P5_6/LCDREF/R13" pad="J12"/>
<connect gate="G$1" pin="P5_7/R23" pad="J11"/>
<connect gate="G$1" pin="P6_0/A0/OA0I0" pad="A4"/>
<connect gate="G$1" pin="P6_1/A1/OA0O" pad="D5"/>
<connect gate="G$1" pin="P6_2/A2/OA0I1" pad="B4"/>
<connect gate="G$1" pin="P6_3/A3/OA1O" pad="B1"/>
<connect gate="G$1" pin="P6_4/A4/OA1I0" pad="B2"/>
<connect gate="G$1" pin="P6_5/A5/OA2O" pad="C2"/>
<connect gate="G$1" pin="P6_6/A6/DAC0/OA2I0" pad="C1"/>
<connect gate="G$1" pin="P6_7/A7/DAC1/SVSIN" pad="C3"/>
<connect gate="G$1" pin="P7_0/UCA0STE/S33" pad="L8"/>
<connect gate="G$1" pin="P7_1/UCA0SIMO/S32" pad="M8"/>
<connect gate="G$1" pin="P7_2/UCA0SOMI/S31" pad="L7"/>
<connect gate="G$1" pin="P7_3/UCA0CLK/S30" pad="H6"/>
<connect gate="G$1" pin="P7_4/S29" pad="M7"/>
<connect gate="G$1" pin="P7_5/S28" pad="J6"/>
<connect gate="G$1" pin="P7_6/S27" pad="L6"/>
<connect gate="G$1" pin="P7_7/S26" pad="M6"/>
<connect gate="G$1" pin="P8_0/S25" pad="J5"/>
<connect gate="G$1" pin="P8_1/S24" pad="H5"/>
<connect gate="G$1" pin="P8_2/S23" pad="M5"/>
<connect gate="G$1" pin="P8_3/S22" pad="L5"/>
<connect gate="G$1" pin="P8_4/S21" pad="G5"/>
<connect gate="G$1" pin="P8_5/S20" pad="M4"/>
<connect gate="G$1" pin="P8_6/S19" pad="L4"/>
<connect gate="G$1" pin="P8_7/S18" pad="H4"/>
<connect gate="G$1" pin="P9_0/S17" pad="M3"/>
<connect gate="G$1" pin="P9_1/S16" pad="L3"/>
<connect gate="G$1" pin="P9_2/S15" pad="K2"/>
<connect gate="G$1" pin="P9_3/S14" pad="M2"/>
<connect gate="G$1" pin="P9_4/S13" pad="L1"/>
<connect gate="G$1" pin="P9_5/S12" pad="K1"/>
<connect gate="G$1" pin="P9_6/S11" pad="G4"/>
<connect gate="G$1" pin="P9_7/S10" pad="J2"/>
<connect gate="G$1" pin="RST/NMI" pad="B5"/>
<connect gate="G$1" pin="TCK" pad="A5"/>
<connect gate="G$1" pin="TDI/TCLK" pad="D6"/>
<connect gate="G$1" pin="TDO/TDI" pad="A6"/>
<connect gate="G$1" pin="TMS" pad="E6"/>
<connect gate="G$1" pin="VEREF+/DAC0" pad="E2"/>
<connect gate="G$1" pin="VREF+" pad="D2"/>
<connect gate="G$1" pin="VREF--/VEREF--" pad="E4"/>
<connect gate="G$1" pin="XIN" pad="D1"/>
<connect gate="G$1" pin="XOUT" pad="E1"/>
<connect gate="G$1" pin="XT2IN" pad="B6"/>
<connect gate="G$1" pin="XT2OUT" pad="B7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430FG4618IZQW"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="61M7852"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS3803" prefix="IC">
<description>&lt;b&gt;Single Voltage Detector&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps3803-01.pdf</description>
<gates>
<gate name="G$1" symbol="TPS3803"/>
</gates>
<devices>
<device name="" package="DCK">
<connects>
<connect gate="G$1" pin="!RESET" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="SENSE" pad="5"/>
<connect gate="G$1" pin="VDD" pad="4"/>
</connects>
<technologies>
<technology name="-01">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS3803-01DCKR"/>
<attribute name="OC_FARNELL" value="1234719"/>
<attribute name="OC_NEWARK" value="77C0392"/>
</technology>
<technology name="H33">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC7226" prefix="IC">
<description>&lt;b&gt;QUADRUPLE 8-BIT DIGITAL-TO-ANALOG CONVERTERS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tlc7226.pdf</description>
<gates>
<gate name="A" symbol="TLC7226"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="A" pin="!WR" pad="15"/>
<connect gate="A" pin="A0" pad="17"/>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="13"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="D3" pad="11"/>
<connect gate="A" pin="D4" pad="10"/>
<connect gate="A" pin="D5" pad="9"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="7"/>
<connect gate="A" pin="DGND" pad="6"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="OUTC" pad="20"/>
<connect gate="A" pin="OUTD" pad="19"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="VDD" pad="18"/>
<connect gate="A" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7226CN"/>
<attribute name="OC_FARNELL" value="8454604"/>
<attribute name="OC_NEWARK" value="36K3647"/>
</technology>
<technology name="I">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TLC7226IN"/>
<attribute name="OC_FARNELL" value="8454620"/>
<attribute name="OC_NEWARK" value="76C7492"/>
</technology>
</technologies>
</device>
<device name="DW" package="SO-20DW">
<connects>
<connect gate="A" pin="!WR" pad="15"/>
<connect gate="A" pin="A0" pad="17"/>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="13"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="D3" pad="11"/>
<connect gate="A" pin="D4" pad="10"/>
<connect gate="A" pin="D5" pad="9"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="7"/>
<connect gate="A" pin="DGND" pad="6"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="OUTC" pad="20"/>
<connect gate="A" pin="OUTD" pad="19"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="VDD" pad="18"/>
<connect gate="A" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="C">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TLC7226CDW"/>
<attribute name="OC_FARNELL" value="9854061"/>
<attribute name="OC_NEWARK" value="35K1223"/>
</technology>
<technology name="I">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TLC7226IDW"/>
<attribute name="OC_FARNELL" value="8454612"/>
<attribute name="OC_NEWARK" value="76C7490"/>
</technology>
</technologies>
</device>
<device name="FK" package="PLCC20">
<connects>
<connect gate="A" pin="!WR" pad="15"/>
<connect gate="A" pin="A0" pad="17"/>
<connect gate="A" pin="A1" pad="16"/>
<connect gate="A" pin="AGND" pad="5"/>
<connect gate="A" pin="D0" pad="14"/>
<connect gate="A" pin="D1" pad="13"/>
<connect gate="A" pin="D2" pad="12"/>
<connect gate="A" pin="D3" pad="11"/>
<connect gate="A" pin="D4" pad="10"/>
<connect gate="A" pin="D5" pad="9"/>
<connect gate="A" pin="D6" pad="8"/>
<connect gate="A" pin="D7" pad="7"/>
<connect gate="A" pin="DGND" pad="6"/>
<connect gate="A" pin="OUTA" pad="2"/>
<connect gate="A" pin="OUTB" pad="1"/>
<connect gate="A" pin="OUTC" pad="20"/>
<connect gate="A" pin="OUTD" pad="19"/>
<connect gate="A" pin="REF" pad="4"/>
<connect gate="A" pin="VDD" pad="18"/>
<connect gate="A" pin="VSS" pad="3"/>
</connects>
<technologies>
<technology name="M">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN65176" prefix="IC">
<description>&lt;b&gt;DIFFERENTIAL BUS TRANSCEIVER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com .. sn65176b.pdf</description>
<gates>
<gate name="E1" symbol="SN65176"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="E1" pin="!RE" pad="2"/>
<connect gate="E1" pin="A" pad="6"/>
<connect gate="E1" pin="B" pad="7"/>
<connect gate="E1" pin="D" pad="4"/>
<connect gate="E1" pin="DE" pad="3"/>
<connect gate="E1" pin="GND" pad="5"/>
<connect gate="E1" pin="R" pad="1"/>
<connect gate="E1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="SN65176BP"/>
<attribute name="OC_FARNELL" value="1755024"/>
<attribute name="OC_NEWARK" value="60K6785"/>
</technology>
</technologies>
</device>
<device name="D" package="SO-08">
<connects>
<connect gate="E1" pin="!RE" pad="2"/>
<connect gate="E1" pin="A" pad="6"/>
<connect gate="E1" pin="B" pad="7"/>
<connect gate="E1" pin="D" pad="4"/>
<connect gate="E1" pin="DE" pad="3"/>
<connect gate="E1" pin="GND" pad="5"/>
<connect gate="E1" pin="R" pad="1"/>
<connect gate="E1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="SN65176BD"/>
<attribute name="OC_FARNELL" value="9589970"/>
<attribute name="OC_NEWARK" value="08F5891"/>
</technology>
</technologies>
</device>
<device name="PS" package="SOP-08">
<connects>
<connect gate="E1" pin="!RE" pad="2"/>
<connect gate="E1" pin="A" pad="6"/>
<connect gate="E1" pin="B" pad="7"/>
<connect gate="E1" pin="D" pad="4"/>
<connect gate="E1" pin="DE" pad="3"/>
<connect gate="E1" pin="GND" pad="5"/>
<connect gate="E1" pin="R" pad="1"/>
<connect gate="E1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OMAP3530_CBB" prefix="IC">
<description>&lt;b&gt;OMAP3530/25 Applications Processor&lt;/b&gt; 600-MHz ARM Cortex?-A8 Core&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 23&lt;/i&gt;&lt;br&gt;
Source: sprm315.bsd</description>
<gates>
<gate name="G$1" symbol="OMAP3530"/>
</gates>
<devices>
<device name="" package="CBB">
<connects>
<connect gate="G$1" pin="BG_TESTOUT" pad="U4"/>
<connect gate="G$1" pin="CAM_D0" pad="AG17"/>
<connect gate="G$1" pin="CAM_D1" pad="AH17"/>
<connect gate="G$1" pin="CAM_D10" pad="B25"/>
<connect gate="G$1" pin="CAM_D11" pad="C26"/>
<connect gate="G$1" pin="CAM_D2" pad="B24"/>
<connect gate="G$1" pin="CAM_D3" pad="C24"/>
<connect gate="G$1" pin="CAM_D4" pad="D24"/>
<connect gate="G$1" pin="CAM_D5" pad="A25"/>
<connect gate="G$1" pin="CAM_D6" pad="K28"/>
<connect gate="G$1" pin="CAM_D7" pad="L28"/>
<connect gate="G$1" pin="CAM_D8" pad="K27"/>
<connect gate="G$1" pin="CAM_D9" pad="L27"/>
<connect gate="G$1" pin="CAM_FLD" pad="C23"/>
<connect gate="G$1" pin="CAM_HS" pad="A24"/>
<connect gate="G$1" pin="CAM_PCLK" pad="C27"/>
<connect gate="G$1" pin="CAM_STROBE" pad="D25"/>
<connect gate="G$1" pin="CAM_VS" pad="A23"/>
<connect gate="G$1" pin="CAM_WEN" pad="B23"/>
<connect gate="G$1" pin="CAM_XCLKA" pad="C25"/>
<connect gate="G$1" pin="CAM_XCLKB" pad="B26"/>
<connect gate="G$1" pin="CAP_VDD_SRAM_CORE" pad="L21"/>
<connect gate="G$1" pin="CAP_VDD_SRAM_MPU_IVA" pad="V4"/>
<connect gate="G$1" pin="CAP_VDD_WKUP" pad="AA15"/>
<connect gate="G$1" pin="DSS_ACBIAS" pad="E27"/>
<connect gate="G$1" pin="DSS_DATA0" pad="AG22"/>
<connect gate="G$1" pin="DSS_DATA1" pad="AH22"/>
<connect gate="G$1" pin="DSS_DATA10" pad="AD28"/>
<connect gate="G$1" pin="DSS_DATA11" pad="AD27"/>
<connect gate="G$1" pin="DSS_DATA12" pad="AB28"/>
<connect gate="G$1" pin="DSS_DATA13" pad="AB27"/>
<connect gate="G$1" pin="DSS_DATA14" pad="AA28"/>
<connect gate="G$1" pin="DSS_DATA15" pad="AA27"/>
<connect gate="G$1" pin="DSS_DATA16" pad="G25"/>
<connect gate="G$1" pin="DSS_DATA17" pad="H27"/>
<connect gate="G$1" pin="DSS_DATA18" pad="H26"/>
<connect gate="G$1" pin="DSS_DATA19" pad="H25"/>
<connect gate="G$1" pin="DSS_DATA2" pad="AG23"/>
<connect gate="G$1" pin="DSS_DATA20" pad="E28"/>
<connect gate="G$1" pin="DSS_DATA21" pad="J26"/>
<connect gate="G$1" pin="DSS_DATA22" pad="AC27"/>
<connect gate="G$1" pin="DSS_DATA23" pad="AC28"/>
<connect gate="G$1" pin="DSS_DATA3" pad="AH23"/>
<connect gate="G$1" pin="DSS_DATA4" pad="AG24"/>
<connect gate="G$1" pin="DSS_DATA5" pad="AH24"/>
<connect gate="G$1" pin="DSS_DATA6" pad="E26"/>
<connect gate="G$1" pin="DSS_DATA7" pad="F28"/>
<connect gate="G$1" pin="DSS_DATA8" pad="F27"/>
<connect gate="G$1" pin="DSS_DATA9" pad="G26"/>
<connect gate="G$1" pin="DSS_HSYNC" pad="D26"/>
<connect gate="G$1" pin="DSS_PCLK" pad="D28"/>
<connect gate="G$1" pin="DSS_VSYNC" pad="D27"/>
<connect gate="G$1" pin="ETK_CLK" pad="AF10"/>
<connect gate="G$1" pin="ETK_CTL" pad="AE10"/>
<connect gate="G$1" pin="ETK_D0" pad="AF11"/>
<connect gate="G$1" pin="ETK_D1" pad="AG12"/>
<connect gate="G$1" pin="ETK_D10" pad="AE7"/>
<connect gate="G$1" pin="ETK_D11" pad="AF7"/>
<connect gate="G$1" pin="ETK_D12" pad="AG7"/>
<connect gate="G$1" pin="ETK_D13" pad="AH7"/>
<connect gate="G$1" pin="ETK_D14" pad="AG8"/>
<connect gate="G$1" pin="ETK_D15" pad="AH8"/>
<connect gate="G$1" pin="ETK_D2" pad="AH12"/>
<connect gate="G$1" pin="ETK_D3" pad="AE13"/>
<connect gate="G$1" pin="ETK_D4" pad="AE11"/>
<connect gate="G$1" pin="ETK_D5" pad="AH9"/>
<connect gate="G$1" pin="ETK_D6" pad="AF13"/>
<connect gate="G$1" pin="ETK_D7" pad="AH14"/>
<connect gate="G$1" pin="ETK_D8" pad="AF9"/>
<connect gate="G$1" pin="ETK_D9" pad="AG9"/>
<connect gate="G$1" pin="GPIO_112" pad="AG19"/>
<connect gate="G$1" pin="GPIO_113" pad="AH19"/>
<connect gate="G$1" pin="GPIO_114" pad="AG18"/>
<connect gate="G$1" pin="GPIO_115" pad="AH18"/>
<connect gate="G$1" pin="GPMC_A1" pad="N4"/>
<connect gate="G$1" pin="GPMC_A10" pad="K3"/>
<connect gate="G$1" pin="GPMC_A2" pad="M4"/>
<connect gate="G$1" pin="GPMC_A3" pad="L4"/>
<connect gate="G$1" pin="GPMC_A4" pad="K4"/>
<connect gate="G$1" pin="GPMC_A5" pad="T3"/>
<connect gate="G$1" pin="GPMC_A6" pad="R3"/>
<connect gate="G$1" pin="GPMC_A7" pad="N3"/>
<connect gate="G$1" pin="GPMC_A8" pad="M3"/>
<connect gate="G$1" pin="GPMC_A9" pad="L3"/>
<connect gate="G$1" pin="GPMC_CLK" pad="T4"/>
<connect gate="G$1" pin="GPMC_D0" pad="K1"/>
<connect gate="G$1" pin="GPMC_D1" pad="L1"/>
<connect gate="G$1" pin="GPMC_D10" pad="P1"/>
<connect gate="G$1" pin="GPMC_D11" pad="R1"/>
<connect gate="G$1" pin="GPMC_D12" pad="R2"/>
<connect gate="G$1" pin="GPMC_D13" pad="T2"/>
<connect gate="G$1" pin="GPMC_D14" pad="W1"/>
<connect gate="G$1" pin="GPMC_D15" pad="Y1"/>
<connect gate="G$1" pin="GPMC_D2" pad="L2"/>
<connect gate="G$1" pin="GPMC_D3" pad="P2"/>
<connect gate="G$1" pin="GPMC_D4" pad="T1"/>
<connect gate="G$1" pin="GPMC_D5" pad="V1"/>
<connect gate="G$1" pin="GPMC_D6" pad="V2"/>
<connect gate="G$1" pin="GPMC_D7" pad="W2"/>
<connect gate="G$1" pin="GPMC_D8" pad="H2"/>
<connect gate="G$1" pin="GPMC_D9" pad="K2"/>
<connect gate="G$1" pin="GPMC_NADV_ALE" pad="F3"/>
<connect gate="G$1" pin="GPMC_NBE0_CLE" pad="G3"/>
<connect gate="G$1" pin="GPMC_NBE1" pad="U3"/>
<connect gate="G$1" pin="GPMC_NCS0" pad="G4"/>
<connect gate="G$1" pin="GPMC_NCS1" pad="H3"/>
<connect gate="G$1" pin="GPMC_NCS2" pad="V8"/>
<connect gate="G$1" pin="GPMC_NCS3" pad="U8"/>
<connect gate="G$1" pin="GPMC_NCS4" pad="T8"/>
<connect gate="G$1" pin="GPMC_NCS5" pad="R8"/>
<connect gate="G$1" pin="GPMC_NCS6" pad="P8"/>
<connect gate="G$1" pin="GPMC_NCS7" pad="N8"/>
<connect gate="G$1" pin="GPMC_NOE" pad="G2"/>
<connect gate="G$1" pin="GPMC_NWE" pad="F4"/>
<connect gate="G$1" pin="GPMC_NWP" pad="H1"/>
<connect gate="G$1" pin="GPMC_WAIT0" pad="M8"/>
<connect gate="G$1" pin="GPMC_WAIT1" pad="L8"/>
<connect gate="G$1" pin="GPMC_WAIT2" pad="K8"/>
<connect gate="G$1" pin="GPMC_WAIT3" pad="J8"/>
<connect gate="G$1" pin="HDQ_SIO" pad="J25"/>
<connect gate="G$1" pin="HSUSB0_CLK" pad="T28"/>
<connect gate="G$1" pin="HSUSB0_DATA0" pad="T27"/>
<connect gate="G$1" pin="HSUSB0_DATA1" pad="U28"/>
<connect gate="G$1" pin="HSUSB0_DATA2" pad="U27"/>
<connect gate="G$1" pin="HSUSB0_DATA3" pad="U26"/>
<connect gate="G$1" pin="HSUSB0_DATA4" pad="U25"/>
<connect gate="G$1" pin="HSUSB0_DATA5" pad="V28"/>
<connect gate="G$1" pin="HSUSB0_DATA6" pad="V27"/>
<connect gate="G$1" pin="HSUSB0_DATA7" pad="V26"/>
<connect gate="G$1" pin="HSUSB0_DIR" pad="R28"/>
<connect gate="G$1" pin="HSUSB0_NXT" pad="T26"/>
<connect gate="G$1" pin="HSUSB0_STP" pad="T25"/>
<connect gate="G$1" pin="I2C1_SCL" pad="J21"/>
<connect gate="G$1" pin="I2C1_SDA" pad="K21"/>
<connect gate="G$1" pin="I2C2_SCL" pad="AF15"/>
<connect gate="G$1" pin="I2C2_SDA" pad="AE15"/>
<connect gate="G$1" pin="I2C3_SCL" pad="AF14"/>
<connect gate="G$1" pin="I2C3_SDA" pad="AG14"/>
<connect gate="G$1" pin="I2C4_SCL" pad="AD26"/>
<connect gate="G$1" pin="I2C4_SDA" pad="AE26"/>
<connect gate="G$1" pin="JTAG_EMU0" pad="AA11"/>
<connect gate="G$1" pin="JTAG_EMU1" pad="AA10"/>
<connect gate="G$1" pin="JTAG_NTRST" pad="AA17"/>
<connect gate="G$1" pin="JTAG_RTCK" pad="AA12"/>
<connect gate="G$1" pin="JTAG_TCK" pad="AA13"/>
<connect gate="G$1" pin="JTAG_TDI" pad="AA20"/>
<connect gate="G$1" pin="JTAG_TDO" pad="AA19"/>
<connect gate="G$1" pin="JTAG_TMS_TSMC" pad="AA18"/>
<connect gate="G$1" pin="MCBSP1_CLKR" pad="Y21"/>
<connect gate="G$1" pin="MCBSP1_CLKX" pad="W21"/>
<connect gate="G$1" pin="MCBSP1_DR" pad="U21"/>
<connect gate="G$1" pin="MCBSP1_DX" pad="V21"/>
<connect gate="G$1" pin="MCBSP1_FSR" pad="AA21"/>
<connect gate="G$1" pin="MCBSP1_FSX" pad="K26"/>
<connect gate="G$1" pin="MCBSP2_CLKX" pad="N21"/>
<connect gate="G$1" pin="MCBSP2_DR" pad="R21"/>
<connect gate="G$1" pin="MCBSP2_DX" pad="M21"/>
<connect gate="G$1" pin="MCBSP2_FSX" pad="P21"/>
<connect gate="G$1" pin="MCBSP3_CLKX" pad="AF5"/>
<connect gate="G$1" pin="MCBSP3_DR" pad="AE6"/>
<connect gate="G$1" pin="MCBSP3_DX" pad="AF6"/>
<connect gate="G$1" pin="MCBSP3_FSX" pad="AE5"/>
<connect gate="G$1" pin="MCBSP4_CLKX" pad="AE1"/>
<connect gate="G$1" pin="MCBSP4_DR" pad="AD1"/>
<connect gate="G$1" pin="MCBSP4_DX" pad="AD2"/>
<connect gate="G$1" pin="MCBSP4_FSX" pad="AC1"/>
<connect gate="G$1" pin="MCBSP_CLKS" pad="T21"/>
<connect gate="G$1" pin="MCSPI1_CLK" pad="AB3"/>
<connect gate="G$1" pin="MCSPI1_CS0" pad="AC2"/>
<connect gate="G$1" pin="MCSPI1_CS1" pad="AC3"/>
<connect gate="G$1" pin="MCSPI1_CS2" pad="AB1"/>
<connect gate="G$1" pin="MCSPI1_CS3" pad="AB2"/>
<connect gate="G$1" pin="MCSPI1_SIMO" pad="AB4"/>
<connect gate="G$1" pin="MCSPI1_SOMI" pad="AA4"/>
<connect gate="G$1" pin="MCSPI2_CLK" pad="AA3"/>
<connect gate="G$1" pin="MCSPI2_CS0" pad="Y4"/>
<connect gate="G$1" pin="MCSPI2_CS1" pad="V3"/>
<connect gate="G$1" pin="MCSPI2_SIMO" pad="Y2"/>
<connect gate="G$1" pin="MCSPI2_SOMI" pad="Y3"/>
<connect gate="G$1" pin="MMC1_CLK" pad="M27"/>
<connect gate="G$1" pin="MMC1_CMD" pad="N28"/>
<connect gate="G$1" pin="MMC1_DAT0" pad="N27"/>
<connect gate="G$1" pin="MMC1_DAT1" pad="N26"/>
<connect gate="G$1" pin="MMC1_DAT2" pad="N25"/>
<connect gate="G$1" pin="MMC1_DAT3" pad="P28"/>
<connect gate="G$1" pin="MMC1_DAT4" pad="P27"/>
<connect gate="G$1" pin="MMC1_DAT5" pad="P26"/>
<connect gate="G$1" pin="MMC1_DAT6" pad="R27"/>
<connect gate="G$1" pin="MMC1_DAT7" pad="R25"/>
<connect gate="G$1" pin="MMC2_CLK" pad="AE2"/>
<connect gate="G$1" pin="MMC2_CMD" pad="AG5"/>
<connect gate="G$1" pin="MMC2_DAT0" pad="AH5"/>
<connect gate="G$1" pin="MMC2_DAT1" pad="AH4"/>
<connect gate="G$1" pin="MMC2_DAT2" pad="AG4"/>
<connect gate="G$1" pin="MMC2_DAT3" pad="AF4"/>
<connect gate="G$1" pin="MMC2_DAT4" pad="AE4"/>
<connect gate="G$1" pin="MMC2_DAT5" pad="AH3"/>
<connect gate="G$1" pin="MMC2_DAT6" pad="AF3"/>
<connect gate="G$1" pin="MMC2_DAT7" pad="AE3"/>
<connect gate="G$1" pin="POP_DDR_VDD_FT@0" pad="A15"/>
<connect gate="G$1" pin="POP_DDR_VDD_FT@1" pad="J28"/>
<connect gate="G$1" pin="POP_DDR_VDD_FT@2" pad="M1"/>
<connect gate="G$1" pin="POP_DDR_VDD_FT@3" pad="AF28"/>
<connect gate="G$1" pin="POP_DDR_VDD_FT@4" pad="AE28"/>
<connect gate="G$1" pin="POP_FLASH_VDD_FT@0" pad="N1"/>
<connect gate="G$1" pin="POP_FLASH_VDD_FT@1" pad="AA1"/>
<connect gate="G$1" pin="POP_FLASH_VDD_FT@2" pad="AF1"/>
<connect gate="G$1" pin="POP_FLASH_VDD_FT@3" pad="AH10"/>
<connect gate="G$1" pin="POP_FLASH_VDD_FT@4" pad="AH15"/>
<connect gate="G$1" pin="POP_FLASH_VPP_FT" pad="AH13"/>
<connect gate="G$1" pin="POP_VSS_FT@0" pad="B15"/>
<connect gate="G$1" pin="POP_VSS_FT@1" pad="J27"/>
<connect gate="G$1" pin="POP_VSS_FT@2" pad="M2"/>
<connect gate="G$1" pin="POP_VSS_FT@3" pad="M26"/>
<connect gate="G$1" pin="POP_VSS_FT@4" pad="N2"/>
<connect gate="G$1" pin="POP_VSS_FT@5" pad="AA2"/>
<connect gate="G$1" pin="POP_VSS_FT@6" pad="AF2"/>
<connect gate="G$1" pin="POP_VSS_FT@7" pad="AF27"/>
<connect gate="G$1" pin="POP_VSS_FT@8" pad="AG10"/>
<connect gate="G$1" pin="POP_VSS_FT@9" pad="AG15"/>
<connect gate="G$1" pin="SDRC_A0" pad="A4"/>
<connect gate="G$1" pin="SDRC_A1" pad="B4"/>
<connect gate="G$1" pin="SDRC_A10" pad="D3"/>
<connect gate="G$1" pin="SDRC_A11" pad="D2"/>
<connect gate="G$1" pin="SDRC_A12" pad="D1"/>
<connect gate="G$1" pin="SDRC_A13" pad="E2"/>
<connect gate="G$1" pin="SDRC_A14" pad="E1"/>
<connect gate="G$1" pin="SDRC_A2" pad="B3"/>
<connect gate="G$1" pin="SDRC_A3" pad="C5"/>
<connect gate="G$1" pin="SDRC_A4" pad="C4"/>
<connect gate="G$1" pin="SDRC_A5" pad="D5"/>
<connect gate="G$1" pin="SDRC_A6" pad="C3"/>
<connect gate="G$1" pin="SDRC_A7" pad="C2"/>
<connect gate="G$1" pin="SDRC_A8" pad="C1"/>
<connect gate="G$1" pin="SDRC_A9" pad="D4"/>
<connect gate="G$1" pin="SDRC_BA0" pad="H9"/>
<connect gate="G$1" pin="SDRC_BA1" pad="H10"/>
<connect gate="G$1" pin="SDRC_CKE0" pad="H16"/>
<connect gate="G$1" pin="SDRC_CKE1" pad="H17"/>
<connect gate="G$1" pin="SDRC_CLK" pad="A13"/>
<connect gate="G$1" pin="SDRC_D0" pad="D6"/>
<connect gate="G$1" pin="SDRC_D1" pad="C6"/>
<connect gate="G$1" pin="SDRC_D10" pad="C15"/>
<connect gate="G$1" pin="SDRC_D11" pad="B16"/>
<connect gate="G$1" pin="SDRC_D12" pad="D17"/>
<connect gate="G$1" pin="SDRC_D13" pad="C17"/>
<connect gate="G$1" pin="SDRC_D14" pad="B17"/>
<connect gate="G$1" pin="SDRC_D15" pad="D18"/>
<connect gate="G$1" pin="SDRC_D16" pad="D11"/>
<connect gate="G$1" pin="SDRC_D17" pad="B10"/>
<connect gate="G$1" pin="SDRC_D18" pad="C11"/>
<connect gate="G$1" pin="SDRC_D19" pad="D12"/>
<connect gate="G$1" pin="SDRC_D2" pad="B6"/>
<connect gate="G$1" pin="SDRC_D20" pad="C12"/>
<connect gate="G$1" pin="SDRC_D21" pad="A11"/>
<connect gate="G$1" pin="SDRC_D22" pad="B13"/>
<connect gate="G$1" pin="SDRC_D23" pad="D14"/>
<connect gate="G$1" pin="SDRC_D24" pad="C18"/>
<connect gate="G$1" pin="SDRC_D25" pad="A19"/>
<connect gate="G$1" pin="SDRC_D26" pad="B19"/>
<connect gate="G$1" pin="SDRC_D27" pad="B20"/>
<connect gate="G$1" pin="SDRC_D28" pad="D20"/>
<connect gate="G$1" pin="SDRC_D29" pad="A21"/>
<connect gate="G$1" pin="SDRC_D3" pad="C8"/>
<connect gate="G$1" pin="SDRC_D30" pad="B21"/>
<connect gate="G$1" pin="SDRC_D31" pad="C21"/>
<connect gate="G$1" pin="SDRC_D4" pad="C9"/>
<connect gate="G$1" pin="SDRC_D5" pad="A7"/>
<connect gate="G$1" pin="SDRC_D6" pad="B9"/>
<connect gate="G$1" pin="SDRC_D7" pad="A9"/>
<connect gate="G$1" pin="SDRC_D8" pad="C14"/>
<connect gate="G$1" pin="SDRC_D9" pad="B14"/>
<connect gate="G$1" pin="SDRC_DM0" pad="B7"/>
<connect gate="G$1" pin="SDRC_DM1" pad="A16"/>
<connect gate="G$1" pin="SDRC_DM2" pad="B11"/>
<connect gate="G$1" pin="SDRC_DM3" pad="C20"/>
<connect gate="G$1" pin="SDRC_DQS0" pad="A6"/>
<connect gate="G$1" pin="SDRC_DQS1" pad="A17"/>
<connect gate="G$1" pin="SDRC_DQS2" pad="A10"/>
<connect gate="G$1" pin="SDRC_DQS3" pad="A20"/>
<connect gate="G$1" pin="SDRC_NCAS" pad="H13"/>
<connect gate="G$1" pin="SDRC_NCLK" pad="A14"/>
<connect gate="G$1" pin="SDRC_NCS0" pad="H11"/>
<connect gate="G$1" pin="SDRC_NCS1" pad="H12"/>
<connect gate="G$1" pin="SDRC_NRAS" pad="H14"/>
<connect gate="G$1" pin="SDRC_NWE" pad="H15"/>
<connect gate="G$1" pin="SYS_32K" pad="AE25"/>
<connect gate="G$1" pin="SYS_BOOT0" pad="AH26"/>
<connect gate="G$1" pin="SYS_BOOT1" pad="AG26"/>
<connect gate="G$1" pin="SYS_BOOT2" pad="AE14"/>
<connect gate="G$1" pin="SYS_BOOT3" pad="AF18"/>
<connect gate="G$1" pin="SYS_BOOT4" pad="AF19"/>
<connect gate="G$1" pin="SYS_BOOT5" pad="AE21"/>
<connect gate="G$1" pin="SYS_BOOT6" pad="AF21"/>
<connect gate="G$1" pin="SYS_CLKOUT1" pad="AG25"/>
<connect gate="G$1" pin="SYS_CLKOUT2" pad="AE22"/>
<connect gate="G$1" pin="SYS_CLKREQ" pad="AF25"/>
<connect gate="G$1" pin="SYS_IPMCSWS" pad="B1"/>
<connect gate="G$1" pin="SYS_NIRQ" pad="AF26"/>
<connect gate="G$1" pin="SYS_NRESPWRON" pad="AH25"/>
<connect gate="G$1" pin="SYS_NRESWARM" pad="AF24"/>
<connect gate="G$1" pin="SYS_OFF_MODE" pad="AF22"/>
<connect gate="G$1" pin="SYS_OPMCSWS" pad="A1"/>
<connect gate="G$1" pin="SYS_XTALIN" pad="AE17"/>
<connect gate="G$1" pin="SYS_XTALOUT" pad="AF17"/>
<connect gate="G$1" pin="TV_OUT1" pad="Y28"/>
<connect gate="G$1" pin="TV_OUT2" pad="W28"/>
<connect gate="G$1" pin="TV_VFB1" pad="Y27"/>
<connect gate="G$1" pin="TV_VFB2" pad="W27"/>
<connect gate="G$1" pin="TV_VREF" pad="W26"/>
<connect gate="G$1" pin="UART1_CTS" pad="W8"/>
<connect gate="G$1" pin="UART1_RTS" pad="AA9"/>
<connect gate="G$1" pin="UART1_RX" pad="Y8"/>
<connect gate="G$1" pin="UART1_TX" pad="AA8"/>
<connect gate="G$1" pin="UART2_CTS" pad="AB26"/>
<connect gate="G$1" pin="UART2_RTS" pad="AB25"/>
<connect gate="G$1" pin="UART2_RX" pad="AD25"/>
<connect gate="G$1" pin="UART2_TX" pad="AA25"/>
<connect gate="G$1" pin="UART3_CTS_RCTX" pad="H18"/>
<connect gate="G$1" pin="UART3_RTS_SD" pad="H19"/>
<connect gate="G$1" pin="UART3_RX_IRRX" pad="H20"/>
<connect gate="G$1" pin="UART3_TX_IRTX" pad="H21"/>
<connect gate="G$1" pin="VDDA_DAC" pad="V25"/>
<connect gate="G$1" pin="VDDS@0" pad="AD3"/>
<connect gate="G$1" pin="VDDS@1" pad="AD4"/>
<connect gate="G$1" pin="VDDS@10" pad="F26"/>
<connect gate="G$1" pin="VDDS@11" pad="AG27"/>
<connect gate="G$1" pin="VDDS@12" pad="AE27"/>
<connect gate="G$1" pin="VDDS@13" pad="AG20"/>
<connect gate="G$1" pin="VDDS@14" pad="H28"/>
<connect gate="G$1" pin="VDDS@15" pad="AG21"/>
<connect gate="G$1" pin="VDDS@16" pad="P25"/>
<connect gate="G$1" pin="VDDS@2" pad="W4"/>
<connect gate="G$1" pin="VDDS@3" pad="AF8"/>
<connect gate="G$1" pin="VDDS@4" pad="AE8"/>
<connect gate="G$1" pin="VDDS@5" pad="AF16"/>
<connect gate="G$1" pin="VDDS@6" pad="AE16"/>
<connect gate="G$1" pin="VDDS@7" pad="AF23"/>
<connect gate="G$1" pin="VDDS@8" pad="AE23"/>
<connect gate="G$1" pin="VDDS@9" pad="F25"/>
<connect gate="G$1" pin="VDDS_DPLL_DLL" pad="K15"/>
<connect gate="G$1" pin="VDDS_DPLL_PER" pad="AA16"/>
<connect gate="G$1" pin="VDDS_MEM@0" pad="U1"/>
<connect gate="G$1" pin="VDDS_MEM@1" pad="J1"/>
<connect gate="G$1" pin="VDDS_MEM@10" pad="A8"/>
<connect gate="G$1" pin="VDDS_MEM@11" pad="B12"/>
<connect gate="G$1" pin="VDDS_MEM@12" pad="A12"/>
<connect gate="G$1" pin="VDDS_MEM@13" pad="D16"/>
<connect gate="G$1" pin="VDDS_MEM@14" pad="C16"/>
<connect gate="G$1" pin="VDDS_MEM@15" pad="B18"/>
<connect gate="G$1" pin="VDDS_MEM@16" pad="A18"/>
<connect gate="G$1" pin="VDDS_MEM@17" pad="B22"/>
<connect gate="G$1" pin="VDDS_MEM@18" pad="A22"/>
<connect gate="G$1" pin="VDDS_MEM@19" pad="G28"/>
<connect gate="G$1" pin="VDDS_MEM@2" pad="F1"/>
<connect gate="G$1" pin="VDDS_MEM@20" pad="C28"/>
<connect gate="G$1" pin="VDDS_MEM@3" pad="J2"/>
<connect gate="G$1" pin="VDDS_MEM@4" pad="F2"/>
<connect gate="G$1" pin="VDDS_MEM@5" pad="R4"/>
<connect gate="G$1" pin="VDDS_MEM@6" pad="B5"/>
<connect gate="G$1" pin="VDDS_MEM@7" pad="A5"/>
<connect gate="G$1" pin="VDDS_MEM@8" pad="AH6"/>
<connect gate="G$1" pin="VDDS_MEM@9" pad="B8"/>
<connect gate="G$1" pin="VDDS_MMC1" pad="K25"/>
<connect gate="G$1" pin="VDDS_SRAM" pad="W16"/>
<connect gate="G$1" pin="VDDS_WKUP_BG" pad="AA14"/>
<connect gate="G$1" pin="VDD_CORE@0" pad="AC4"/>
<connect gate="G$1" pin="VDD_CORE@1" pad="J4"/>
<connect gate="G$1" pin="VDD_CORE@10" pad="W18"/>
<connect gate="G$1" pin="VDD_CORE@11" pad="K18"/>
<connect gate="G$1" pin="VDD_CORE@12" pad="J18"/>
<connect gate="G$1" pin="VDD_CORE@13" pad="AE19"/>
<connect gate="G$1" pin="VDD_CORE@14" pad="Y19"/>
<connect gate="G$1" pin="VDD_CORE@15" pad="U19"/>
<connect gate="G$1" pin="VDD_CORE@16" pad="T19"/>
<connect gate="G$1" pin="VDD_CORE@17" pad="N19"/>
<connect gate="G$1" pin="VDD_CORE@18" pad="M19"/>
<connect gate="G$1" pin="VDD_CORE@19" pad="J19"/>
<connect gate="G$1" pin="VDD_CORE@2" pad="H4"/>
<connect gate="G$1" pin="VDD_CORE@20" pad="Y20"/>
<connect gate="G$1" pin="VDD_CORE@21" pad="W20"/>
<connect gate="G$1" pin="VDD_CORE@22" pad="V20"/>
<connect gate="G$1" pin="VDD_CORE@23" pad="U20"/>
<connect gate="G$1" pin="VDD_CORE@24" pad="P20"/>
<connect gate="G$1" pin="VDD_CORE@25" pad="N20"/>
<connect gate="G$1" pin="VDD_CORE@26" pad="K20"/>
<connect gate="G$1" pin="VDD_CORE@27" pad="J20"/>
<connect gate="G$1" pin="VDD_CORE@28" pad="D22"/>
<connect gate="G$1" pin="VDD_CORE@29" pad="D23"/>
<connect gate="G$1" pin="VDD_CORE@3" pad="D8"/>
<connect gate="G$1" pin="VDD_CORE@30" pad="AE24"/>
<connect gate="G$1" pin="VDD_CORE@31" pad="M25"/>
<connect gate="G$1" pin="VDD_CORE@32" pad="L25"/>
<connect gate="G$1" pin="VDD_CORE@33" pad="E25"/>
<connect gate="G$1" pin="VDD_CORE@4" pad="AE9"/>
<connect gate="G$1" pin="VDD_CORE@5" pad="D9"/>
<connect gate="G$1" pin="VDD_CORE@6" pad="D15"/>
<connect gate="G$1" pin="VDD_CORE@7" pad="Y16"/>
<connect gate="G$1" pin="VDD_CORE@8" pad="AE18"/>
<connect gate="G$1" pin="VDD_CORE@9" pad="Y18"/>
<connect gate="G$1" pin="VDD_MPU_IVA@0" pad="Y9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@1" pad="W9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@10" pad="R10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@11" pad="N10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@12" pad="M10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@13" pad="L10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@14" pad="J10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@15" pad="Y11"/>
<connect gate="G$1" pin="VDD_MPU_IVA@16" pad="W11"/>
<connect gate="G$1" pin="VDD_MPU_IVA@17" pad="K11"/>
<connect gate="G$1" pin="VDD_MPU_IVA@18" pad="J11"/>
<connect gate="G$1" pin="VDD_MPU_IVA@19" pad="W12"/>
<connect gate="G$1" pin="VDD_MPU_IVA@2" pad="T9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@20" pad="K13"/>
<connect gate="G$1" pin="VDD_MPU_IVA@21" pad="Y14"/>
<connect gate="G$1" pin="VDD_MPU_IVA@22" pad="K14"/>
<connect gate="G$1" pin="VDD_MPU_IVA@23" pad="J14"/>
<connect gate="G$1" pin="VDD_MPU_IVA@24" pad="Y15"/>
<connect gate="G$1" pin="VDD_MPU_IVA@25" pad="W15"/>
<connect gate="G$1" pin="VDD_MPU_IVA@26" pad="J15"/>
<connect gate="G$1" pin="VDD_MPU_IVA@3" pad="R9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@4" pad="M9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@5" pad="L9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@6" pad="J9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@7" pad="Y10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@8" pad="U10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@9" pad="T10"/>
<connect gate="G$1" pin="VPP" pad="G1"/>
<connect gate="G$1" pin="VSS@0" pad="AG2"/>
<connect gate="G$1" pin="VSS@1" pad="U2"/>
<connect gate="G$1" pin="VSS@10" pad="E4"/>
<connect gate="G$1" pin="VSS@11" pad="AG6"/>
<connect gate="G$1" pin="VSS@12" pad="D7"/>
<connect gate="G$1" pin="VSS@13" pad="C7"/>
<connect gate="G$1" pin="VSS@14" pad="V9"/>
<connect gate="G$1" pin="VSS@15" pad="U9"/>
<connect gate="G$1" pin="VSS@16" pad="P9"/>
<connect gate="G$1" pin="VSS@17" pad="N9"/>
<connect gate="G$1" pin="VSS@18" pad="K9"/>
<connect gate="G$1" pin="VSS@19" pad="W10"/>
<connect gate="G$1" pin="VSS@2" pad="B2"/>
<connect gate="G$1" pin="VSS@20" pad="V10"/>
<connect gate="G$1" pin="VSS@21" pad="P10"/>
<connect gate="G$1" pin="VSS@22" pad="K10"/>
<connect gate="G$1" pin="VSS@23" pad="D10"/>
<connect gate="G$1" pin="VSS@24" pad="C10"/>
<connect gate="G$1" pin="VSS@25" pad="AF12"/>
<connect gate="G$1" pin="VSS@26" pad="AE12"/>
<connect gate="G$1" pin="VSS@27" pad="Y12"/>
<connect gate="G$1" pin="VSS@28" pad="K12"/>
<connect gate="G$1" pin="VSS@29" pad="J12"/>
<connect gate="G$1" pin="VSS@3" pad="AG3"/>
<connect gate="G$1" pin="VSS@30" pad="Y13"/>
<connect gate="G$1" pin="VSS@31" pad="W13"/>
<connect gate="G$1" pin="VSS@32" pad="J13"/>
<connect gate="G$1" pin="VSS@33" pad="D13"/>
<connect gate="G$1" pin="VSS@34" pad="C13"/>
<connect gate="G$1" pin="VSS@35" pad="W14"/>
<connect gate="G$1" pin="VSS@36" pad="K16"/>
<connect gate="G$1" pin="VSS@37" pad="J16"/>
<connect gate="G$1" pin="VSS@38" pad="Y17"/>
<connect gate="G$1" pin="VSS@39" pad="W17"/>
<connect gate="G$1" pin="VSS@4" pad="W3"/>
<connect gate="G$1" pin="VSS@40" pad="K17"/>
<connect gate="G$1" pin="VSS@41" pad="J17"/>
<connect gate="G$1" pin="VSS@42" pad="W19"/>
<connect gate="G$1" pin="VSS@43" pad="V19"/>
<connect gate="G$1" pin="VSS@44" pad="R19"/>
<connect gate="G$1" pin="VSS@45" pad="P19"/>
<connect gate="G$1" pin="VSS@46" pad="L19"/>
<connect gate="G$1" pin="VSS@47" pad="K19"/>
<connect gate="G$1" pin="VSS@48" pad="D19"/>
<connect gate="G$1" pin="VSS@49" pad="C19"/>
<connect gate="G$1" pin="VSS@5" pad="P3"/>
<connect gate="G$1" pin="VSS@50" pad="AF20"/>
<connect gate="G$1" pin="VSS@51" pad="AE20"/>
<connect gate="G$1" pin="VSS@52" pad="T20"/>
<connect gate="G$1" pin="VSS@53" pad="R20"/>
<connect gate="G$1" pin="VSS@54" pad="M20"/>
<connect gate="G$1" pin="VSS@55" pad="L20"/>
<connect gate="G$1" pin="VSS@56" pad="D21"/>
<connect gate="G$1" pin="VSS@57" pad="C22"/>
<connect gate="G$1" pin="VSS@58" pad="AC25"/>
<connect gate="G$1" pin="VSS@59" pad="Y25"/>
<connect gate="G$1" pin="VSS@6" pad="J3"/>
<connect gate="G$1" pin="VSS@60" pad="W25"/>
<connect gate="G$1" pin="VSS@61" pad="AC26"/>
<connect gate="G$1" pin="VSS@62" pad="R26"/>
<connect gate="G$1" pin="VSS@63" pad="L26"/>
<connect gate="G$1" pin="VSS@64" pad="A26"/>
<connect gate="G$1" pin="VSS@65" pad="G27"/>
<connect gate="G$1" pin="VSS@66" pad="B27"/>
<connect gate="G$1" pin="VSS@67" pad="AA26"/>
<connect gate="G$1" pin="VSS@68" pad="M28"/>
<connect gate="G$1" pin="VSS@69" pad="AG16"/>
<connect gate="G$1" pin="VSS@7" pad="E3"/>
<connect gate="G$1" pin="VSS@70" pad="AH21"/>
<connect gate="G$1" pin="VSS@8" pad="A3"/>
<connect gate="G$1" pin="VSS@9" pad="P4"/>
<connect gate="G$1" pin="VSSA_DAC" pad="Y26"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1660215"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OMAP3530_CUS" prefix="IC">
<description>&lt;b&gt;OMAP 3530/25 Applications Processor&lt;/b&gt; 600-MHz ARM Cortex?-A8 Core&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 23&lt;/i&gt;&lt;br&gt;
Source: sprm314.bsd</description>
<gates>
<gate name="G$1" symbol="SPRM314"/>
</gates>
<devices>
<device name="" package="CUS">
<connects>
<connect gate="G$1" pin="BG_TESTOUT" pad="AD1"/>
<connect gate="G$1" pin="CAM_D0" pad="AB18"/>
<connect gate="G$1" pin="CAM_D1" pad="AC18"/>
<connect gate="G$1" pin="CAM_D10" pad="F21"/>
<connect gate="G$1" pin="CAM_D11" pad="G21"/>
<connect gate="G$1" pin="CAM_D2" pad="G19"/>
<connect gate="G$1" pin="CAM_D3" pad="F19"/>
<connect gate="G$1" pin="CAM_D4" pad="G20"/>
<connect gate="G$1" pin="CAM_D5" pad="B21"/>
<connect gate="G$1" pin="CAM_D6" pad="L24"/>
<connect gate="G$1" pin="CAM_D7" pad="K24"/>
<connect gate="G$1" pin="CAM_D8" pad="J23"/>
<connect gate="G$1" pin="CAM_D9" pad="K23"/>
<connect gate="G$1" pin="CAM_FLD" pad="H24"/>
<connect gate="G$1" pin="CAM_HS" pad="A22"/>
<connect gate="G$1" pin="CAM_PCLK" pad="J19"/>
<connect gate="G$1" pin="CAM_STROBE" pad="J20"/>
<connect gate="G$1" pin="CAM_VS" pad="E18"/>
<connect gate="G$1" pin="CAM_WEN" pad="F18"/>
<connect gate="G$1" pin="CAM_XCLKA" pad="B22"/>
<connect gate="G$1" pin="CAM_XCLKB" pad="C22"/>
<connect gate="G$1" pin="CAP_VDD_SRAM_CORE" pad="H17"/>
<connect gate="G$1" pin="CAP_VDD_SRAM_MPU_IVA" pad="U8"/>
<connect gate="G$1" pin="CAP_VDD_WKUP" pad="Y12"/>
<connect gate="G$1" pin="DSS_ACBIAS" pad="J21"/>
<connect gate="G$1" pin="DSS_DATA0" pad="AC19"/>
<connect gate="G$1" pin="DSS_DATA1" pad="AB19"/>
<connect gate="G$1" pin="DSS_DATA10" pad="AC22"/>
<connect gate="G$1" pin="DSS_DATA11" pad="AC23"/>
<connect gate="G$1" pin="DSS_DATA12" pad="AB22"/>
<connect gate="G$1" pin="DSS_DATA13" pad="Y22"/>
<connect gate="G$1" pin="DSS_DATA14" pad="W22"/>
<connect gate="G$1" pin="DSS_DATA15" pad="V22"/>
<connect gate="G$1" pin="DSS_DATA16" pad="J22"/>
<connect gate="G$1" pin="DSS_DATA17" pad="G23"/>
<connect gate="G$1" pin="DSS_DATA18" pad="G24"/>
<connect gate="G$1" pin="DSS_DATA19" pad="H23"/>
<connect gate="G$1" pin="DSS_DATA2" pad="AD20"/>
<connect gate="G$1" pin="DSS_DATA20" pad="D23"/>
<connect gate="G$1" pin="DSS_DATA21" pad="K22"/>
<connect gate="G$1" pin="DSS_DATA22" pad="V21"/>
<connect gate="G$1" pin="DSS_DATA23" pad="W21"/>
<connect gate="G$1" pin="DSS_DATA3" pad="AC20"/>
<connect gate="G$1" pin="DSS_DATA4" pad="AD21"/>
<connect gate="G$1" pin="DSS_DATA5" pad="AC21"/>
<connect gate="G$1" pin="DSS_DATA6" pad="D24"/>
<connect gate="G$1" pin="DSS_DATA7" pad="E23"/>
<connect gate="G$1" pin="DSS_DATA8" pad="E24"/>
<connect gate="G$1" pin="DSS_DATA9" pad="F23"/>
<connect gate="G$1" pin="DSS_HSYNC" pad="E22"/>
<connect gate="G$1" pin="DSS_PCLK" pad="G22"/>
<connect gate="G$1" pin="DSS_VSYNC" pad="F22"/>
<connect gate="G$1" pin="ETK_CLK" pad="AC1"/>
<connect gate="G$1" pin="ETK_CTL" pad="AD3"/>
<connect gate="G$1" pin="ETK_D0" pad="AD6"/>
<connect gate="G$1" pin="ETK_D1" pad="AC6"/>
<connect gate="G$1" pin="ETK_D10" pad="AC3"/>
<connect gate="G$1" pin="ETK_D11" pad="AC9"/>
<connect gate="G$1" pin="ETK_D12" pad="AC10"/>
<connect gate="G$1" pin="ETK_D13" pad="AD11"/>
<connect gate="G$1" pin="ETK_D14" pad="AC11"/>
<connect gate="G$1" pin="ETK_D15" pad="AD12"/>
<connect gate="G$1" pin="ETK_D2" pad="AC7"/>
<connect gate="G$1" pin="ETK_D3" pad="AD8"/>
<connect gate="G$1" pin="ETK_D4" pad="AC5"/>
<connect gate="G$1" pin="ETK_D5" pad="AD2"/>
<connect gate="G$1" pin="ETK_D6" pad="AC8"/>
<connect gate="G$1" pin="ETK_D7" pad="AD9"/>
<connect gate="G$1" pin="ETK_D8" pad="AC4"/>
<connect gate="G$1" pin="ETK_D9" pad="AD5"/>
<connect gate="G$1" pin="GPMC_A1" pad="K4"/>
<connect gate="G$1" pin="GPMC_A10" pad="G2"/>
<connect gate="G$1" pin="GPMC_A2" pad="K3"/>
<connect gate="G$1" pin="GPMC_A3" pad="K2"/>
<connect gate="G$1" pin="GPMC_A4" pad="J4"/>
<connect gate="G$1" pin="GPMC_A5" pad="J3"/>
<connect gate="G$1" pin="GPMC_A6" pad="J2"/>
<connect gate="G$1" pin="GPMC_A7" pad="J1"/>
<connect gate="G$1" pin="GPMC_A8" pad="H1"/>
<connect gate="G$1" pin="GPMC_A9" pad="H2"/>
<connect gate="G$1" pin="GPMC_CLK" pad="W2"/>
<connect gate="G$1" pin="GPMC_D0" pad="L2"/>
<connect gate="G$1" pin="GPMC_D1" pad="M1"/>
<connect gate="G$1" pin="GPMC_D10" pad="U1"/>
<connect gate="G$1" pin="GPMC_D11" pad="R3"/>
<connect gate="G$1" pin="GPMC_D12" pad="T3"/>
<connect gate="G$1" pin="GPMC_D13" pad="U2"/>
<connect gate="G$1" pin="GPMC_D14" pad="V1"/>
<connect gate="G$1" pin="GPMC_D15" pad="V2"/>
<connect gate="G$1" pin="GPMC_D2" pad="M2"/>
<connect gate="G$1" pin="GPMC_D3" pad="N2"/>
<connect gate="G$1" pin="GPMC_D4" pad="M3"/>
<connect gate="G$1" pin="GPMC_D5" pad="P1"/>
<connect gate="G$1" pin="GPMC_D6" pad="P2"/>
<connect gate="G$1" pin="GPMC_D7" pad="R1"/>
<connect gate="G$1" pin="GPMC_D8" pad="R2"/>
<connect gate="G$1" pin="GPMC_D9" pad="T2"/>
<connect gate="G$1" pin="GPMC_NADV_ALE" pad="F1"/>
<connect gate="G$1" pin="GPMC_NBE0_CLE" pad="K5"/>
<connect gate="G$1" pin="GPMC_NBE1" pad="L1"/>
<connect gate="G$1" pin="GPMC_NCS0" pad="E2"/>
<connect gate="G$1" pin="GPMC_NCS3" pad="D2"/>
<connect gate="G$1" pin="GPMC_NCS4" pad="F4"/>
<connect gate="G$1" pin="GPMC_NCS5" pad="G5"/>
<connect gate="G$1" pin="GPMC_NCS6" pad="F3"/>
<connect gate="G$1" pin="GPMC_NCS7" pad="G4"/>
<connect gate="G$1" pin="GPMC_NOE" pad="F2"/>
<connect gate="G$1" pin="GPMC_NWE" pad="G3"/>
<connect gate="G$1" pin="GPMC_NWP" pad="E1"/>
<connect gate="G$1" pin="GPMC_WAIT0" pad="C1"/>
<connect gate="G$1" pin="GPMC_WAIT3" pad="C2"/>
<connect gate="G$1" pin="HDQ_SIO" pad="A24"/>
<connect gate="G$1" pin="HSUSB0_CLK" pad="R21"/>
<connect gate="G$1" pin="HSUSB0_DATA0" pad="T24"/>
<connect gate="G$1" pin="HSUSB0_DATA1" pad="T23"/>
<connect gate="G$1" pin="HSUSB0_DATA2" pad="U24"/>
<connect gate="G$1" pin="HSUSB0_DATA3" pad="U23"/>
<connect gate="G$1" pin="HSUSB0_DATA4" pad="W24"/>
<connect gate="G$1" pin="HSUSB0_DATA5" pad="V23"/>
<connect gate="G$1" pin="HSUSB0_DATA6" pad="W23"/>
<connect gate="G$1" pin="HSUSB0_DATA7" pad="T22"/>
<connect gate="G$1" pin="HSUSB0_DIR" pad="P23"/>
<connect gate="G$1" pin="HSUSB0_NXT" pad="R22"/>
<connect gate="G$1" pin="HSUSB0_STP" pad="R23"/>
<connect gate="G$1" pin="I2C1_SCL" pad="K20"/>
<connect gate="G$1" pin="I2C1_SDA" pad="K21"/>
<connect gate="G$1" pin="I2C2_SCL" pad="AC15"/>
<connect gate="G$1" pin="I2C2_SDA" pad="AC14"/>
<connect gate="G$1" pin="I2C3_SCL" pad="AC13"/>
<connect gate="G$1" pin="I2C3_SDA" pad="AC12"/>
<connect gate="G$1" pin="I2C4_SCL" pad="Y16"/>
<connect gate="G$1" pin="I2C4_SDA" pad="Y15"/>
<connect gate="G$1" pin="JTAG_EMU0" pad="AC24"/>
<connect gate="G$1" pin="JTAG_EMU1" pad="AD24"/>
<connect gate="G$1" pin="JTAG_NTRST" pad="AB7"/>
<connect gate="G$1" pin="JTAG_RTCK" pad="AA7"/>
<connect gate="G$1" pin="JTAG_TCK" pad="AB6"/>
<connect gate="G$1" pin="JTAG_TDI" pad="AB10"/>
<connect gate="G$1" pin="JTAG_TDO" pad="AB9"/>
<connect gate="G$1" pin="JTAG_TMS_TSMC" pad="AA9"/>
<connect gate="G$1" pin="MCBSP1_CLKR" pad="W19"/>
<connect gate="G$1" pin="MCBSP1_CLKX" pad="V18"/>
<connect gate="G$1" pin="MCBSP1_DR" pad="Y18"/>
<connect gate="G$1" pin="MCBSP1_DX" pad="W18"/>
<connect gate="G$1" pin="MCBSP1_FSR" pad="AB20"/>
<connect gate="G$1" pin="MCBSP1_FSX" pad="AA19"/>
<connect gate="G$1" pin="MCBSP2_CLKX" pad="T21"/>
<connect gate="G$1" pin="MCBSP2_DR" pad="V19"/>
<connect gate="G$1" pin="MCBSP2_DX" pad="R20"/>
<connect gate="G$1" pin="MCBSP2_FSX" pad="V20"/>
<connect gate="G$1" pin="MCBSP3_CLKX" pad="W4"/>
<connect gate="G$1" pin="MCBSP3_DR" pad="V5"/>
<connect gate="G$1" pin="MCBSP3_DX" pad="V6"/>
<connect gate="G$1" pin="MCBSP3_FSX" pad="V4"/>
<connect gate="G$1" pin="MCBSP_CLKS" pad="AA18"/>
<connect gate="G$1" pin="MCSPI1_CLK" pad="T5"/>
<connect gate="G$1" pin="MCSPI1_CS0" pad="T6"/>
<connect gate="G$1" pin="MCSPI1_CS3" pad="R5"/>
<connect gate="G$1" pin="MCSPI1_SIMO" pad="R4"/>
<connect gate="G$1" pin="MCSPI1_SOMI" pad="T4"/>
<connect gate="G$1" pin="MCSPI2_CLK" pad="N5"/>
<connect gate="G$1" pin="MCSPI2_CS0" pad="M5"/>
<connect gate="G$1" pin="MCSPI2_CS1" pad="M4"/>
<connect gate="G$1" pin="MCSPI2_SIMO" pad="N4"/>
<connect gate="G$1" pin="MCSPI2_SOMI" pad="N3"/>
<connect gate="G$1" pin="MMC1_CLK" pad="M23"/>
<connect gate="G$1" pin="MMC1_CMD" pad="L23"/>
<connect gate="G$1" pin="MMC1_DAT0" pad="M22"/>
<connect gate="G$1" pin="MMC1_DAT1" pad="M21"/>
<connect gate="G$1" pin="MMC1_DAT2" pad="M20"/>
<connect gate="G$1" pin="MMC1_DAT3" pad="N23"/>
<connect gate="G$1" pin="MMC1_DAT4" pad="N22"/>
<connect gate="G$1" pin="MMC1_DAT5" pad="N21"/>
<connect gate="G$1" pin="MMC1_DAT6" pad="N20"/>
<connect gate="G$1" pin="MMC1_DAT7" pad="P24"/>
<connect gate="G$1" pin="MMC2_CLK" pad="Y1"/>
<connect gate="G$1" pin="MMC2_CMD" pad="AB5"/>
<connect gate="G$1" pin="MMC2_DAT0" pad="AB3"/>
<connect gate="G$1" pin="MMC2_DAT1" pad="Y3"/>
<connect gate="G$1" pin="MMC2_DAT2" pad="W3"/>
<connect gate="G$1" pin="MMC2_DAT3" pad="V3"/>
<connect gate="G$1" pin="MMC2_DAT4" pad="AB2"/>
<connect gate="G$1" pin="MMC2_DAT5" pad="AA2"/>
<connect gate="G$1" pin="MMC2_DAT6" pad="Y2"/>
<connect gate="G$1" pin="MMC2_DAT7" pad="AA1"/>
<connect gate="G$1" pin="SDRC_A0" pad="A4"/>
<connect gate="G$1" pin="SDRC_A1" pad="B4"/>
<connect gate="G$1" pin="SDRC_A10" pad="E7"/>
<connect gate="G$1" pin="SDRC_A11" pad="G6"/>
<connect gate="G$1" pin="SDRC_A12" pad="G7"/>
<connect gate="G$1" pin="SDRC_A13" pad="F7"/>
<connect gate="G$1" pin="SDRC_A14" pad="F9"/>
<connect gate="G$1" pin="SDRC_A2" pad="D6"/>
<connect gate="G$1" pin="SDRC_A3" pad="B3"/>
<connect gate="G$1" pin="SDRC_A4" pad="B2"/>
<connect gate="G$1" pin="SDRC_A5" pad="C3"/>
<connect gate="G$1" pin="SDRC_A6" pad="E3"/>
<connect gate="G$1" pin="SDRC_A7" pad="F6"/>
<connect gate="G$1" pin="SDRC_A8" pad="E10"/>
<connect gate="G$1" pin="SDRC_A9" pad="E9"/>
<connect gate="G$1" pin="SDRC_BA0" pad="C18"/>
<connect gate="G$1" pin="SDRC_BA1" pad="D18"/>
<connect gate="G$1" pin="SDRC_CKE0" pad="B20"/>
<connect gate="G$1" pin="SDRC_CKE1" pad="C20"/>
<connect gate="G$1" pin="SDRC_CLK" pad="A10"/>
<connect gate="G$1" pin="SDRC_D0" pad="D7"/>
<connect gate="G$1" pin="SDRC_D1" pad="C5"/>
<connect gate="G$1" pin="SDRC_D10" pad="B12"/>
<connect gate="G$1" pin="SDRC_D11" pad="D13"/>
<connect gate="G$1" pin="SDRC_D12" pad="C13"/>
<connect gate="G$1" pin="SDRC_D13" pad="B14"/>
<connect gate="G$1" pin="SDRC_D14" pad="A14"/>
<connect gate="G$1" pin="SDRC_D15" pad="B15"/>
<connect gate="G$1" pin="SDRC_D16" pad="C9"/>
<connect gate="G$1" pin="SDRC_D17" pad="E12"/>
<connect gate="G$1" pin="SDRC_D18" pad="B8"/>
<connect gate="G$1" pin="SDRC_D19" pad="B9"/>
<connect gate="G$1" pin="SDRC_D2" pad="C6"/>
<connect gate="G$1" pin="SDRC_D20" pad="C10"/>
<connect gate="G$1" pin="SDRC_D21" pad="B10"/>
<connect gate="G$1" pin="SDRC_D22" pad="D12"/>
<connect gate="G$1" pin="SDRC_D23" pad="E13"/>
<connect gate="G$1" pin="SDRC_D24" pad="E15"/>
<connect gate="G$1" pin="SDRC_D25" pad="D15"/>
<connect gate="G$1" pin="SDRC_D26" pad="C15"/>
<connect gate="G$1" pin="SDRC_D27" pad="B16"/>
<connect gate="G$1" pin="SDRC_D28" pad="C16"/>
<connect gate="G$1" pin="SDRC_D29" pad="D16"/>
<connect gate="G$1" pin="SDRC_D3" pad="B5"/>
<connect gate="G$1" pin="SDRC_D30" pad="B17"/>
<connect gate="G$1" pin="SDRC_D31" pad="B18"/>
<connect gate="G$1" pin="SDRC_D4" pad="D9"/>
<connect gate="G$1" pin="SDRC_D5" pad="D10"/>
<connect gate="G$1" pin="SDRC_D6" pad="C7"/>
<connect gate="G$1" pin="SDRC_D7" pad="B7"/>
<connect gate="G$1" pin="SDRC_D8" pad="B11"/>
<connect gate="G$1" pin="SDRC_D9" pad="C12"/>
<connect gate="G$1" pin="SDRC_DM0" pad="B6"/>
<connect gate="G$1" pin="SDRC_DM1" pad="B13"/>
<connect gate="G$1" pin="SDRC_DM2" pad="A7"/>
<connect gate="G$1" pin="SDRC_DM3" pad="A16"/>
<connect gate="G$1" pin="SDRC_DQS0" pad="A5"/>
<connect gate="G$1" pin="SDRC_DQS1" pad="A13"/>
<connect gate="G$1" pin="SDRC_DQS2" pad="A8"/>
<connect gate="G$1" pin="SDRC_DQS3" pad="A17"/>
<connect gate="G$1" pin="SDRC_NCAS" pad="C19"/>
<connect gate="G$1" pin="SDRC_NCLK" pad="A11"/>
<connect gate="G$1" pin="SDRC_NCS0" pad="A19"/>
<connect gate="G$1" pin="SDRC_NCS1" pad="B19"/>
<connect gate="G$1" pin="SDRC_NRAS" pad="D19"/>
<connect gate="G$1" pin="SDRC_NWE" pad="A20"/>
<connect gate="G$1" pin="SYS_32K" pad="AA16"/>
<connect gate="G$1" pin="SYS_BOOT0" pad="AB12"/>
<connect gate="G$1" pin="SYS_BOOT1" pad="AC16"/>
<connect gate="G$1" pin="SYS_BOOT2" pad="AD17"/>
<connect gate="G$1" pin="SYS_BOOT3" pad="AD18"/>
<connect gate="G$1" pin="SYS_BOOT4" pad="AC17"/>
<connect gate="G$1" pin="SYS_BOOT5" pad="AB16"/>
<connect gate="G$1" pin="SYS_BOOT6" pad="AA15"/>
<connect gate="G$1" pin="SYS_CLKOUT1" pad="Y7"/>
<connect gate="G$1" pin="SYS_CLKOUT2" pad="AA6"/>
<connect gate="G$1" pin="SYS_CLKREQ" pad="Y13"/>
<connect gate="G$1" pin="SYS_IPMCSWS" pad="A1"/>
<connect gate="G$1" pin="SYS_NIRQ" pad="W16"/>
<connect gate="G$1" pin="SYS_NRESPWRON" pad="AA10"/>
<connect gate="G$1" pin="SYS_NRESWARM" pad="Y10"/>
<connect gate="G$1" pin="SYS_OFF_MODE" pad="AD23"/>
<connect gate="G$1" pin="SYS_OPMCSWS" pad="A2"/>
<connect gate="G$1" pin="SYS_XTALIN" pad="AD15"/>
<connect gate="G$1" pin="SYS_XTALOUT" pad="AD14"/>
<connect gate="G$1" pin="TV_OUT1" pad="AB24"/>
<connect gate="G$1" pin="TV_OUT2" pad="AA23"/>
<connect gate="G$1" pin="TV_VFB1" pad="AB23"/>
<connect gate="G$1" pin="TV_VFB2" pad="Y23"/>
<connect gate="G$1" pin="TV_VREF" pad="Y24"/>
<connect gate="G$1" pin="UART1_CTS" pad="AC2"/>
<connect gate="G$1" pin="UART1_RTS" pad="W6"/>
<connect gate="G$1" pin="UART1_RX" pad="V7"/>
<connect gate="G$1" pin="UART1_TX" pad="W7"/>
<connect gate="G$1" pin="UART3_CTS_RCTX" pad="A23"/>
<connect gate="G$1" pin="UART3_RTS_SD" pad="B23"/>
<connect gate="G$1" pin="UART3_RX_IRRX" pad="B24"/>
<connect gate="G$1" pin="UART3_TX_IRTX" pad="C23"/>
<connect gate="G$1" pin="VDDA_DAC" pad="AB13"/>
<connect gate="G$1" pin="VDDS@0" pad="Y9"/>
<connect gate="G$1" pin="VDDS@1" pad="W10"/>
<connect gate="G$1" pin="VDDS@10" pad="M18"/>
<connect gate="G$1" pin="VDDS@11" pad="M17"/>
<connect gate="G$1" pin="VDDS@12" pad="H8"/>
<connect gate="G$1" pin="VDDS@2" pad="W9"/>
<connect gate="G$1" pin="VDDS@3" pad="V10"/>
<connect gate="G$1" pin="VDDS@4" pad="V9"/>
<connect gate="G$1" pin="VDDS@5" pad="U10"/>
<connect gate="G$1" pin="VDDS@6" pad="N19"/>
<connect gate="G$1" pin="VDDS@7" pad="N18"/>
<connect gate="G$1" pin="VDDS@8" pad="N17"/>
<connect gate="G$1" pin="VDDS@9" pad="M19"/>
<connect gate="G$1" pin="VDDS_DPLL_DLL" pad="G18"/>
<connect gate="G$1" pin="VDDS_DPLL_PER" pad="U17"/>
<connect gate="G$1" pin="VDDS_MEM@0" pad="K8"/>
<connect gate="G$1" pin="VDDS_MEM@1" pad="K7"/>
<connect gate="G$1" pin="VDDS_MEM@10" pad="F15"/>
<connect gate="G$1" pin="VDDS_MEM@11" pad="E16"/>
<connect gate="G$1" pin="VDDS_MEM@2" pad="K6"/>
<connect gate="G$1" pin="VDDS_MEM@3" pad="J8"/>
<connect gate="G$1" pin="VDDS_MEM@4" pad="J7"/>
<connect gate="G$1" pin="VDDS_MEM@5" pad="J6"/>
<connect gate="G$1" pin="VDDS_MEM@6" pad="H15"/>
<connect gate="G$1" pin="VDDS_MEM@7" pad="G16"/>
<connect gate="G$1" pin="VDDS_MEM@8" pad="G15"/>
<connect gate="G$1" pin="VDDS_MEM@9" pad="F16"/>
<connect gate="G$1" pin="VDDS_MMC1" pad="N24"/>
<connect gate="G$1" pin="VDDS_SRAM" pad="AA12"/>
<connect gate="G$1" pin="VDDS_WKUP_BG" pad="AA13"/>
<connect gate="G$1" pin="VDD_CORE@0" pad="T20"/>
<connect gate="G$1" pin="VDD_CORE@1" pad="T19"/>
<connect gate="G$1" pin="VDD_CORE@10" pad="L14"/>
<connect gate="G$1" pin="VDD_CORE@11" pad="K19"/>
<connect gate="G$1" pin="VDD_CORE@12" pad="K18"/>
<connect gate="G$1" pin="VDD_CORE@13" pad="K17"/>
<connect gate="G$1" pin="VDD_CORE@14" pad="J18"/>
<connect gate="G$1" pin="VDD_CORE@15" pad="J17"/>
<connect gate="G$1" pin="VDD_CORE@16" pad="H13"/>
<connect gate="G$1" pin="VDD_CORE@17" pad="H12"/>
<connect gate="G$1" pin="VDD_CORE@18" pad="G13"/>
<connect gate="G$1" pin="VDD_CORE@19" pad="G12"/>
<connect gate="G$1" pin="VDD_CORE@2" pad="T18"/>
<connect gate="G$1" pin="VDD_CORE@20" pad="F13"/>
<connect gate="G$1" pin="VDD_CORE@21" pad="F12"/>
<connect gate="G$1" pin="VDD_CORE@3" pad="T17"/>
<connect gate="G$1" pin="VDD_CORE@4" pad="R19"/>
<connect gate="G$1" pin="VDD_CORE@5" pad="R18"/>
<connect gate="G$1" pin="VDD_CORE@6" pad="R17"/>
<connect gate="G$1" pin="VDD_CORE@7" pad="M15"/>
<connect gate="G$1" pin="VDD_CORE@8" pad="M14"/>
<connect gate="G$1" pin="VDD_CORE@9" pad="L15"/>
<connect gate="G$1" pin="VDD_MPU_IVA@0" pad="W13"/>
<connect gate="G$1" pin="VDD_MPU_IVA@1" pad="W12"/>
<connect gate="G$1" pin="VDD_MPU_IVA@10" pad="R6"/>
<connect gate="G$1" pin="VDD_MPU_IVA@11" pad="N8"/>
<connect gate="G$1" pin="VDD_MPU_IVA@12" pad="N7"/>
<connect gate="G$1" pin="VDD_MPU_IVA@13" pad="N6"/>
<connect gate="G$1" pin="VDD_MPU_IVA@14" pad="M12"/>
<connect gate="G$1" pin="VDD_MPU_IVA@15" pad="M8"/>
<connect gate="G$1" pin="VDD_MPU_IVA@16" pad="M7"/>
<connect gate="G$1" pin="VDD_MPU_IVA@17" pad="M6"/>
<connect gate="G$1" pin="VDD_MPU_IVA@18" pad="L12"/>
<connect gate="G$1" pin="VDD_MPU_IVA@19" pad="L11"/>
<connect gate="G$1" pin="VDD_MPU_IVA@2" pad="V13"/>
<connect gate="G$1" pin="VDD_MPU_IVA@20" pad="J10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@21" pad="J9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@22" pad="H10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@23" pad="H9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@24" pad="G10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@25" pad="G9"/>
<connect gate="G$1" pin="VDD_MPU_IVA@26" pad="F10"/>
<connect gate="G$1" pin="VDD_MPU_IVA@3" pad="V12"/>
<connect gate="G$1" pin="VDD_MPU_IVA@4" pad="U13"/>
<connect gate="G$1" pin="VDD_MPU_IVA@5" pad="U12"/>
<connect gate="G$1" pin="VDD_MPU_IVA@6" pad="T8"/>
<connect gate="G$1" pin="VDD_MPU_IVA@7" pad="T7"/>
<connect gate="G$1" pin="VDD_MPU_IVA@8" pad="R8"/>
<connect gate="G$1" pin="VDD_MPU_IVA@9" pad="R7"/>
<connect gate="G$1" pin="VPP" pad="B1"/>
<connect gate="G$1" pin="VSS@0" pad="W15"/>
<connect gate="G$1" pin="VSS@1" pad="V16"/>
<connect gate="G$1" pin="VSS@10" pad="T14"/>
<connect gate="G$1" pin="VSS@11" pad="T13"/>
<connect gate="G$1" pin="VSS@12" pad="T12"/>
<connect gate="G$1" pin="VSS@13" pad="T11"/>
<connect gate="G$1" pin="VSS@14" pad="T10"/>
<connect gate="G$1" pin="VSS@15" pad="T9"/>
<connect gate="G$1" pin="VSS@16" pad="R15"/>
<connect gate="G$1" pin="VSS@17" pad="R14"/>
<connect gate="G$1" pin="VSS@18" pad="R11"/>
<connect gate="G$1" pin="VSS@19" pad="R10"/>
<connect gate="G$1" pin="VSS@2" pad="V15"/>
<connect gate="G$1" pin="VSS@20" pad="P17"/>
<connect gate="G$1" pin="VSS@21" pad="P15"/>
<connect gate="G$1" pin="VSS@22" pad="P14"/>
<connect gate="G$1" pin="VSS@23" pad="P13"/>
<connect gate="G$1" pin="VSS@24" pad="P12"/>
<connect gate="G$1" pin="VSS@25" pad="P11"/>
<connect gate="G$1" pin="VSS@26" pad="P10"/>
<connect gate="G$1" pin="VSS@27" pad="P8"/>
<connect gate="G$1" pin="VSS@28" pad="N16"/>
<connect gate="G$1" pin="VSS@29" pad="N15"/>
<connect gate="G$1" pin="VSS@3" pad="U16"/>
<connect gate="G$1" pin="VSS@30" pad="N14"/>
<connect gate="G$1" pin="VSS@31" pad="N13"/>
<connect gate="G$1" pin="VSS@32" pad="N12"/>
<connect gate="G$1" pin="VSS@33" pad="N11"/>
<connect gate="G$1" pin="VSS@34" pad="N10"/>
<connect gate="G$1" pin="VSS@35" pad="N9"/>
<connect gate="G$1" pin="VSS@36" pad="M16"/>
<connect gate="G$1" pin="VSS@37" pad="M13"/>
<connect gate="G$1" pin="VSS@38" pad="M11"/>
<connect gate="G$1" pin="VSS@39" pad="M10"/>
<connect gate="G$1" pin="VSS@4" pad="U15"/>
<connect gate="G$1" pin="VSS@40" pad="M9"/>
<connect gate="G$1" pin="VSS@41" pad="L17"/>
<connect gate="G$1" pin="VSS@42" pad="L13"/>
<connect gate="G$1" pin="VSS@43" pad="L10"/>
<connect gate="G$1" pin="VSS@44" pad="L8"/>
<connect gate="G$1" pin="VSS@45" pad="K15"/>
<connect gate="G$1" pin="VSS@46" pad="K14"/>
<connect gate="G$1" pin="VSS@47" pad="K11"/>
<connect gate="G$1" pin="VSS@48" pad="K10"/>
<connect gate="G$1" pin="VSS@49" pad="J16"/>
<connect gate="G$1" pin="VSS@5" pad="U14"/>
<connect gate="G$1" pin="VSS@50" pad="J15"/>
<connect gate="G$1" pin="VSS@51" pad="J14"/>
<connect gate="G$1" pin="VSS@52" pad="J13"/>
<connect gate="G$1" pin="VSS@53" pad="J12"/>
<connect gate="G$1" pin="VSS@54" pad="J11"/>
<connect gate="G$1" pin="VSS@55" pad="H16"/>
<connect gate="G$1" pin="VSS@56" pad="H14"/>
<connect gate="G$1" pin="VSS@57" pad="H11"/>
<connect gate="G$1" pin="VSS@6" pad="U11"/>
<connect gate="G$1" pin="VSS@7" pad="U9"/>
<connect gate="G$1" pin="VSS@8" pad="T16"/>
<connect gate="G$1" pin="VSS@9" pad="T15"/>
<connect gate="G$1" pin="VSSA_DAC" pad="AB15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS65023" prefix="IC">
<description>&lt;b&gt;POWER MANAGEMENT IC FOR LI-ION POWERED SYSTEMS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps65023.pdf</description>
<gates>
<gate name="G$1" symbol="TPS65023"/>
<gate name="-EXP" symbol="EXP17"/>
</gates>
<devices>
<device name="" package="QFN40-5X5">
<connects>
<connect gate="-EXP" pin="EXP" pad="EXP"/>
<connect gate="-EXP" pin="EXP16@1" pad="EXP@1"/>
<connect gate="-EXP" pin="EXP16@10" pad="EXP@10"/>
<connect gate="-EXP" pin="EXP16@11" pad="EXP@11"/>
<connect gate="-EXP" pin="EXP16@12" pad="EXP@12"/>
<connect gate="-EXP" pin="EXP16@13" pad="EXP@13"/>
<connect gate="-EXP" pin="EXP16@14" pad="EXP@14"/>
<connect gate="-EXP" pin="EXP16@15" pad="EXP@15"/>
<connect gate="-EXP" pin="EXP16@16" pad="EXP@16"/>
<connect gate="-EXP" pin="EXP16@2" pad="EXP@2"/>
<connect gate="-EXP" pin="EXP16@3" pad="EXP@3"/>
<connect gate="-EXP" pin="EXP16@4" pad="EXP@4"/>
<connect gate="-EXP" pin="EXP16@5" pad="EXP@5"/>
<connect gate="-EXP" pin="EXP16@6" pad="EXP@6"/>
<connect gate="-EXP" pin="EXP16@7" pad="EXP@7"/>
<connect gate="-EXP" pin="EXP16@8" pad="EXP@8"/>
<connect gate="-EXP" pin="EXP16@9" pad="EXP@9"/>
<connect gate="G$1" pin="!HOT_RESET" pad="11"/>
<connect gate="G$1" pin="!INT" pad="28"/>
<connect gate="G$1" pin="!LOWBAT" pad="21"/>
<connect gate="G$1" pin="!PWRFAIL" pad="31"/>
<connect gate="G$1" pin="!RESPWRON" pad="27"/>
<connect gate="G$1" pin="AGND1" pad="40"/>
<connect gate="G$1" pin="AGND2" pad="17"/>
<connect gate="G$1" pin="DCDC1_EN" pad="25"/>
<connect gate="G$1" pin="DCDC2_EN" pad="24"/>
<connect gate="G$1" pin="DCDC3_EN" pad="23"/>
<connect gate="G$1" pin="DEFDCDC1" pad="10"/>
<connect gate="G$1" pin="DEFDCDC2" pad="32"/>
<connect gate="G$1" pin="DEFDCDC3" pad="1"/>
<connect gate="G$1" pin="DEFLDO1" pad="12"/>
<connect gate="G$1" pin="DEFLDO2" pad="13"/>
<connect gate="G$1" pin="L1" pad="7"/>
<connect gate="G$1" pin="L2" pad="35"/>
<connect gate="G$1" pin="L3" pad="4"/>
<connect gate="G$1" pin="LDO_EN" pad="22"/>
<connect gate="G$1" pin="LOWBAT_SNS" pad="39"/>
<connect gate="G$1" pin="PGND1" pad="8"/>
<connect gate="G$1" pin="PGND2" pad="34"/>
<connect gate="G$1" pin="PGND3" pad="3"/>
<connect gate="G$1" pin="PWRFAIL_SNS" pad="38"/>
<connect gate="G$1" pin="SCLK" pad="30"/>
<connect gate="G$1" pin="SDAT" pad="29"/>
<connect gate="G$1" pin="TRESPWRON" pad="26"/>
<connect gate="G$1" pin="VBACKUP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="37"/>
<connect gate="G$1" pin="VDCDC1" pad="9"/>
<connect gate="G$1" pin="VDCDC2" pad="33"/>
<connect gate="G$1" pin="VDCDC3" pad="2"/>
<connect gate="G$1" pin="VINDCDC1" pad="6"/>
<connect gate="G$1" pin="VINDCDC2" pad="36"/>
<connect gate="G$1" pin="VINDCDC3" pad="5"/>
<connect gate="G$1" pin="VINLDO" pad="19"/>
<connect gate="G$1" pin="VLDO1" pad="20"/>
<connect gate="G$1" pin="VLDO2" pad="18"/>
<connect gate="G$1" pin="VRTC" pad="16"/>
<connect gate="G$1" pin="VSYSIN" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS65023RSBR"/>
<attribute name="OC_FARNELL" value="1652451"/>
<attribute name="OC_NEWARK" value="22M1826"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS65020" prefix="IC">
<description>&lt;b&gt;POWER MANAGEMENT IC FOR LI-ION POWERED SYSTEMS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps65020.pdf</description>
<gates>
<gate name="G$1" symbol="TPS65020"/>
<gate name="-EXP" symbol="EXP-16"/>
</gates>
<devices>
<device name="" package="QFN40-6X6">
<connects>
<connect gate="-EXP" pin="EXP16@1" pad="EXP@1"/>
<connect gate="-EXP" pin="EXP16@10" pad="EXP@10"/>
<connect gate="-EXP" pin="EXP16@11" pad="EXP@11"/>
<connect gate="-EXP" pin="EXP16@12" pad="EXP@12"/>
<connect gate="-EXP" pin="EXP16@13" pad="EXP@13"/>
<connect gate="-EXP" pin="EXP16@14" pad="EXP@14"/>
<connect gate="-EXP" pin="EXP16@15" pad="EXP@15"/>
<connect gate="-EXP" pin="EXP16@16" pad="EXP@16"/>
<connect gate="-EXP" pin="EXP16@2" pad="EXP@2"/>
<connect gate="-EXP" pin="EXP16@3" pad="EXP@3"/>
<connect gate="-EXP" pin="EXP16@4" pad="EXP@4"/>
<connect gate="-EXP" pin="EXP16@5" pad="EXP@5"/>
<connect gate="-EXP" pin="EXP16@6" pad="EXP@6"/>
<connect gate="-EXP" pin="EXP16@7" pad="EXP@7"/>
<connect gate="-EXP" pin="EXP16@8" pad="EXP@8"/>
<connect gate="-EXP" pin="EXP16@9" pad="EXP@9"/>
<connect gate="G$1" pin="!HOT_RESET" pad="11"/>
<connect gate="G$1" pin="!INT" pad="28"/>
<connect gate="G$1" pin="!LOWBAT" pad="21"/>
<connect gate="G$1" pin="!PWRFAIL" pad="31"/>
<connect gate="G$1" pin="!RESPWRON" pad="27"/>
<connect gate="G$1" pin="AGND1" pad="40"/>
<connect gate="G$1" pin="AGND2" pad="17"/>
<connect gate="G$1" pin="DCDC1_EN" pad="25"/>
<connect gate="G$1" pin="DCDC2_EN" pad="24"/>
<connect gate="G$1" pin="DCDC3_EN" pad="23"/>
<connect gate="G$1" pin="DEFDCDC1" pad="10"/>
<connect gate="G$1" pin="DEFDCDC2" pad="32"/>
<connect gate="G$1" pin="DEFDCDC3" pad="1"/>
<connect gate="G$1" pin="L1" pad="7"/>
<connect gate="G$1" pin="L2" pad="35"/>
<connect gate="G$1" pin="L3" pad="4"/>
<connect gate="G$1" pin="LDO_EN" pad="22"/>
<connect gate="G$1" pin="LOWBAT_SNS" pad="39"/>
<connect gate="G$1" pin="PB_IN" pad="12"/>
<connect gate="G$1" pin="PB_OUT" pad="13"/>
<connect gate="G$1" pin="PGND1" pad="8"/>
<connect gate="G$1" pin="PGND2" pad="34"/>
<connect gate="G$1" pin="PGND3" pad="3"/>
<connect gate="G$1" pin="PWRFAIL_SNS" pad="38"/>
<connect gate="G$1" pin="SCLK" pad="30"/>
<connect gate="G$1" pin="SDAT" pad="29"/>
<connect gate="G$1" pin="TRESPWRON" pad="26"/>
<connect gate="G$1" pin="VBACKUP" pad="15"/>
<connect gate="G$1" pin="VCC" pad="37"/>
<connect gate="G$1" pin="VDCDC1" pad="9"/>
<connect gate="G$1" pin="VDCDC2" pad="33"/>
<connect gate="G$1" pin="VDCDC3" pad="2"/>
<connect gate="G$1" pin="VINDCDC1" pad="6"/>
<connect gate="G$1" pin="VINDCDC2" pad="36"/>
<connect gate="G$1" pin="VINDCDC3" pad="5"/>
<connect gate="G$1" pin="VINLDO" pad="19"/>
<connect gate="G$1" pin="VLDO1" pad="20"/>
<connect gate="G$1" pin="VLDO2" pad="18"/>
<connect gate="G$1" pin="VRTC" pad="16"/>
<connect gate="G$1" pin="VSYSIN" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TPS65020RHAT"/>
<attribute name="OC_FARNELL" value="1412603"/>
<attribute name="OC_NEWARK" value="61K1903"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24120" prefix="IC">
<description>&lt;b&gt;SINGLE-CHIP SWITCHMODE, LI-ION AND LI-POLYMER CHARGE-MANAGEMENT IC&lt;/b&gt;&lt;p&gt;
WITH ENHANCED EMI PERFORMANCE(bqSWITCHER)&lt;br&gt;
Source: www.ti.com .. TI-bq24125.pdf</description>
<gates>
<gate name="G$1" symbol="BQ24120-1"/>
<gate name="-EXP" symbol="EXP"/>
</gates>
<devices>
<device name="" package="QFN20_3,5X4,5">
<connects>
<connect gate="-EXP" pin="1" pad="EXP@1"/>
<connect gate="-EXP" pin="10" pad="EXP@9"/>
<connect gate="-EXP" pin="11" pad="EXP@10"/>
<connect gate="-EXP" pin="12" pad="EXP@11"/>
<connect gate="-EXP" pin="13" pad="EXP@12"/>
<connect gate="-EXP" pin="2" pad="EXP@2"/>
<connect gate="-EXP" pin="3" pad="EXP@3"/>
<connect gate="-EXP" pin="4" pad="EXP@4"/>
<connect gate="-EXP" pin="5" pad="EXP@5"/>
<connect gate="-EXP" pin="6" pad="EXP@6"/>
<connect gate="-EXP" pin="7" pad="EXP"/>
<connect gate="-EXP" pin="8" pad="EXP@7"/>
<connect gate="-EXP" pin="9" pad="EXP@8"/>
<connect gate="G$1" pin="!CE" pad="16"/>
<connect gate="G$1" pin="!PG" pad="5"/>
<connect gate="G$1" pin="BAT" pad="14"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="4"/>
<connect gate="G$1" pin="ISET1" pad="8"/>
<connect gate="G$1" pin="ISET2" pad="9"/>
<connect gate="G$1" pin="NC" pad="13"/>
<connect gate="G$1" pin="OUT@1" pad="1"/>
<connect gate="G$1" pin="OUT@2" pad="20"/>
<connect gate="G$1" pin="PGND@1" pad="17"/>
<connect gate="G$1" pin="PGND@2" pad="18"/>
<connect gate="G$1" pin="SNS" pad="15"/>
<connect gate="G$1" pin="STAT1" pad="2"/>
<connect gate="G$1" pin="STAT2" pad="19"/>
<connect gate="G$1" pin="TS" pad="12"/>
<connect gate="G$1" pin="TTC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VSS" pad="10"/>
<connect gate="G$1" pin="VTSB" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ24120RHLTG4"/>
<attribute name="OC_FARNELL" value="1230453"/>
<attribute name="OC_NEWARK" value="12M9386"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24123" prefix="IC">
<description>&lt;b&gt;SINGLE-CHIP SWITCHMODE, LI-ION AND LI-POLYMER CHARGE-MANAGEMENT IC&lt;/b&gt;&lt;p&gt;
WITH ENHANCED EMI PERFORMANCE(bqSWITCHER)&lt;br&gt;
Source: www.ti.com .. TI-bq24125.pdf</description>
<gates>
<gate name="G$1" symbol="BQ24123"/>
<gate name="-EXP" symbol="EXP"/>
</gates>
<devices>
<device name="" package="QFN20_3,5X4,5">
<connects>
<connect gate="-EXP" pin="1" pad="EXP@1"/>
<connect gate="-EXP" pin="10" pad="EXP@9"/>
<connect gate="-EXP" pin="11" pad="EXP@10"/>
<connect gate="-EXP" pin="12" pad="EXP@11"/>
<connect gate="-EXP" pin="13" pad="EXP@12"/>
<connect gate="-EXP" pin="2" pad="EXP@2"/>
<connect gate="-EXP" pin="3" pad="EXP@3"/>
<connect gate="-EXP" pin="4" pad="EXP@4"/>
<connect gate="-EXP" pin="5" pad="EXP@5"/>
<connect gate="-EXP" pin="6" pad="EXP@6"/>
<connect gate="-EXP" pin="7" pad="EXP"/>
<connect gate="-EXP" pin="8" pad="EXP@7"/>
<connect gate="-EXP" pin="9" pad="EXP@8"/>
<connect gate="G$1" pin="!CE" pad="16"/>
<connect gate="G$1" pin="!PG" pad="5"/>
<connect gate="G$1" pin="BAT" pad="14"/>
<connect gate="G$1" pin="CELLS" pad="13"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="4"/>
<connect gate="G$1" pin="ISET1" pad="8"/>
<connect gate="G$1" pin="ISET2" pad="9"/>
<connect gate="G$1" pin="OUT@1" pad="1"/>
<connect gate="G$1" pin="OUT@2" pad="20"/>
<connect gate="G$1" pin="PGND@1" pad="17"/>
<connect gate="G$1" pin="PGND@2" pad="18"/>
<connect gate="G$1" pin="SNS" pad="15"/>
<connect gate="G$1" pin="STAT1" pad="2"/>
<connect gate="G$1" pin="STAT2" pad="19"/>
<connect gate="G$1" pin="TS" pad="12"/>
<connect gate="G$1" pin="TTC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VSS" pad="10"/>
<connect gate="G$1" pin="VTSB" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ24123RHLT"/>
<attribute name="OC_FARNELL" value="1407131"/>
<attribute name="OC_NEWARK" value="84K0851"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24125" prefix="IC">
<description>&lt;b&gt;SINGLE-CHIP SWITCHMODE, LI-ION AND LI-POLYMER CHARGE-MANAGEMENT IC&lt;/b&gt;&lt;p&gt;
WITH ENHANCED EMI PERFORMANCE(bqSWITCHER)&lt;br&gt;
Source: www.ti.com .. TI-bq24125.pdf</description>
<gates>
<gate name="G$1" symbol="BQ24125"/>
<gate name="-EXP" symbol="EXP"/>
</gates>
<devices>
<device name="" package="QFN20_3,5X4,5">
<connects>
<connect gate="-EXP" pin="1" pad="EXP@1"/>
<connect gate="-EXP" pin="10" pad="EXP@9"/>
<connect gate="-EXP" pin="11" pad="EXP@10"/>
<connect gate="-EXP" pin="12" pad="EXP@11"/>
<connect gate="-EXP" pin="13" pad="EXP@12"/>
<connect gate="-EXP" pin="2" pad="EXP@2"/>
<connect gate="-EXP" pin="3" pad="EXP@3"/>
<connect gate="-EXP" pin="4" pad="EXP@4"/>
<connect gate="-EXP" pin="5" pad="EXP@5"/>
<connect gate="-EXP" pin="6" pad="EXP@6"/>
<connect gate="-EXP" pin="7" pad="EXP"/>
<connect gate="-EXP" pin="8" pad="EXP@7"/>
<connect gate="-EXP" pin="9" pad="EXP@8"/>
<connect gate="G$1" pin="!CE" pad="16"/>
<connect gate="G$1" pin="!PG" pad="5"/>
<connect gate="G$1" pin="BAT" pad="14"/>
<connect gate="G$1" pin="FB" pad="13"/>
<connect gate="G$1" pin="IN1" pad="3"/>
<connect gate="G$1" pin="IN2" pad="4"/>
<connect gate="G$1" pin="ISET1" pad="8"/>
<connect gate="G$1" pin="ISET2" pad="9"/>
<connect gate="G$1" pin="OUT@1" pad="1"/>
<connect gate="G$1" pin="OUT@2" pad="20"/>
<connect gate="G$1" pin="PGND@1" pad="17"/>
<connect gate="G$1" pin="PGND@2" pad="18"/>
<connect gate="G$1" pin="SNS" pad="15"/>
<connect gate="G$1" pin="STAT1" pad="2"/>
<connect gate="G$1" pin="STAT2" pad="19"/>
<connect gate="G$1" pin="TS" pad="12"/>
<connect gate="G$1" pin="TTC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="6"/>
<connect gate="G$1" pin="VSS" pad="10"/>
<connect gate="G$1" pin="VTSB" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ24125RHLR"/>
<attribute name="OC_FARNELL" value="1536712"/>
<attribute name="OC_NEWARK" value="71M2021"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ27500" prefix="IC">
<description>&lt;b&gt;System-Side Impedance Track? Fuel Gauge&lt;/b&gt;&lt;p&gt;
Source: bq27500-v100.pdf</description>
<gates>
<gate name="G$1" symbol="BQ27500"/>
<gate name="P" symbol="PWPD9"/>
</gates>
<devices>
<device name="" package="DRZ">
<connects>
<connect gate="G$1" pin="!BAT_GD" pad="12"/>
<connect gate="G$1" pin="BAT" pad="4"/>
<connect gate="G$1" pin="BAT_LOW" pad="1"/>
<connect gate="G$1" pin="BI/TOUT" pad="2"/>
<connect gate="G$1" pin="NC" pad="9"/>
<connect gate="G$1" pin="SCL" pad="11"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="SRN" pad="8"/>
<connect gate="G$1" pin="SRP" pad="7"/>
<connect gate="G$1" pin="TS" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="P" pin="PWPD@1" pad="EXP@1"/>
<connect gate="P" pin="PWPD@2" pad="EXP@2"/>
<connect gate="P" pin="PWPD@3" pad="EXP@3"/>
<connect gate="P" pin="PWPD@4" pad="EXP@4"/>
<connect gate="P" pin="PWPD@5" pad="EXP@5"/>
<connect gate="P" pin="PWPD@6" pad="EXP@6"/>
<connect gate="P" pin="PWPD@7" pad="EXP@7"/>
<connect gate="P" pin="PWPD@8" pad="EXP@8"/>
<connect gate="P" pin="PWPD@9" pad="EXP@9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ27500DRZR"/>
<attribute name="OC_FARNELL" value="1561320"/>
<attribute name="OC_NEWARK" value="84M8746"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ27501" prefix="IC">
<description>&lt;b&gt;System-Side Impedance Track? Fuel Gauge&lt;/b&gt;&lt;p&gt;
Source: bq27500-v100.pdf</description>
<gates>
<gate name="G$1" symbol="BQ27501"/>
<gate name="P" symbol="PWPD9"/>
</gates>
<devices>
<device name="" package="DRZ">
<connects>
<connect gate="G$1" pin="!BAT_GD" pad="12"/>
<connect gate="G$1" pin="BAT" pad="4"/>
<connect gate="G$1" pin="BAT_LOW" pad="1"/>
<connect gate="G$1" pin="BI/TOUT" pad="2"/>
<connect gate="G$1" pin="RID" pad="9"/>
<connect gate="G$1" pin="SCL" pad="11"/>
<connect gate="G$1" pin="SDA" pad="10"/>
<connect gate="G$1" pin="SRN" pad="8"/>
<connect gate="G$1" pin="SRP" pad="7"/>
<connect gate="G$1" pin="TS" pad="3"/>
<connect gate="G$1" pin="VCC" pad="5"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="P" pin="PWPD@1" pad="EXP@1"/>
<connect gate="P" pin="PWPD@2" pad="EXP@2"/>
<connect gate="P" pin="PWPD@3" pad="EXP@3"/>
<connect gate="P" pin="PWPD@4" pad="EXP@4"/>
<connect gate="P" pin="PWPD@5" pad="EXP@5"/>
<connect gate="P" pin="PWPD@6" pad="EXP@6"/>
<connect gate="P" pin="PWPD@7" pad="EXP@7"/>
<connect gate="P" pin="PWPD@8" pad="EXP@8"/>
<connect gate="P" pin="PWPD@9" pad="EXP@9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ27501DRZT"/>
<attribute name="OC_FARNELL" value="1710789"/>
<attribute name="OC_NEWARK" value="50P9379"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO7241" prefix="IC">
<description>&lt;b&gt;HIGH SPEED QUAD DIGITAL ISOLATORS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/iso7240m.pdf</description>
<gates>
<gate name="G$1" symbol="ISO7241"/>
</gates>
<devices>
<device name="" package="SO-16DW">
<connects>
<connect gate="G$1" pin="EN1" pad="7"/>
<connect gate="G$1" pin="EN2" pad="10"/>
<connect gate="G$1" pin="GND1@1" pad="2"/>
<connect gate="G$1" pin="GND1@2" pad="8"/>
<connect gate="G$1" pin="GND2@1" pad="15"/>
<connect gate="G$1" pin="GND2@2" pad="9"/>
<connect gate="G$1" pin="INA" pad="3"/>
<connect gate="G$1" pin="INB" pad="4"/>
<connect gate="G$1" pin="INC" pad="5"/>
<connect gate="G$1" pin="IND" pad="11"/>
<connect gate="G$1" pin="OUTA" pad="14"/>
<connect gate="G$1" pin="OUTB" pad="13"/>
<connect gate="G$1" pin="OUTC" pad="12"/>
<connect gate="G$1" pin="OUTD" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7241CDW"/>
<attribute name="OC_FARNELL" value="1575372"/>
<attribute name="OC_NEWARK" value="73M3155"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO7240" prefix="IC">
<description>&lt;b&gt;HIGH SPEED QUAD DIGITAL ISOLATORS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/iso7240m.pdf</description>
<gates>
<gate name="G$1" symbol="ISO7240"/>
</gates>
<devices>
<device name="" package="SO-16DW">
<connects>
<connect gate="G$1" pin="EN" pad="10"/>
<connect gate="G$1" pin="GND1@1" pad="2"/>
<connect gate="G$1" pin="GND1@2" pad="8"/>
<connect gate="G$1" pin="GND2@1" pad="15"/>
<connect gate="G$1" pin="GND2@2" pad="9"/>
<connect gate="G$1" pin="INA" pad="3"/>
<connect gate="G$1" pin="INB" pad="4"/>
<connect gate="G$1" pin="INC" pad="5"/>
<connect gate="G$1" pin="IND" pad="6"/>
<connect gate="G$1" pin="NC" pad="7"/>
<connect gate="G$1" pin="OUTA" pad="14"/>
<connect gate="G$1" pin="OUTB" pad="13"/>
<connect gate="G$1" pin="OUTC" pad="12"/>
<connect gate="G$1" pin="OUTD" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7240MDW"/>
<attribute name="OC_FARNELL" value="1755124"/>
<attribute name="OC_NEWARK" value="58M0385"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO7242" prefix="IC">
<description>&lt;b&gt;HIGH SPEED QUAD DIGITAL ISOLATORS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/iso7240m.pdf</description>
<gates>
<gate name="G$1" symbol="ISO7242"/>
</gates>
<devices>
<device name="" package="SO-16DW">
<connects>
<connect gate="G$1" pin="EN1" pad="7"/>
<connect gate="G$1" pin="EN2" pad="10"/>
<connect gate="G$1" pin="GND1@1" pad="2"/>
<connect gate="G$1" pin="GND1@2" pad="8"/>
<connect gate="G$1" pin="GND2@1" pad="15"/>
<connect gate="G$1" pin="GND2@2" pad="9"/>
<connect gate="G$1" pin="INA" pad="3"/>
<connect gate="G$1" pin="INB" pad="4"/>
<connect gate="G$1" pin="INC" pad="12"/>
<connect gate="G$1" pin="IND" pad="11"/>
<connect gate="G$1" pin="OUTA" pad="14"/>
<connect gate="G$1" pin="OUTB" pad="13"/>
<connect gate="G$1" pin="OUTC" pad="5"/>
<connect gate="G$1" pin="OUTD" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7242MDW"/>
<attribute name="OC_FARNELL" value="1755127"/>
<attribute name="OC_NEWARK" value="73M3163"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO7221" prefix="IC">
<description>&lt;b&gt;DUAL DIGITAL ISOLATORS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/iso7221a.pdf</description>
<gates>
<gate name="G$1" symbol="ISO7221"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="INA" pad="7"/>
<connect gate="G$1" pin="INB" pad="3"/>
<connect gate="G$1" pin="OUTA" pad="2"/>
<connect gate="G$1" pin="OUTB" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="8"/>
</connects>
<technologies>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7221AD"/>
<attribute name="OC_FARNELL" value="1390651"/>
<attribute name="OC_NEWARK" value="48M0672"/>
</technology>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7221BD"/>
<attribute name="OC_FARNELL" value="1600639"/>
<attribute name="OC_NEWARK" value="94M7889"/>
</technology>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7221CD"/>
<attribute name="OC_FARNELL" value="1390645"/>
<attribute name="OC_NEWARK" value="61M6993"/>
</technology>
<technology name="M">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7221MD"/>
<attribute name="OC_FARNELL" value="1390647"/>
<attribute name="OC_NEWARK" value="48M0676"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO7220" prefix="IC">
<description>&lt;b&gt;DUAL DIGITAL ISOLATORS&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/iso7221a.pdf</description>
<gates>
<gate name="G$1" symbol="ISO7220"/>
</gates>
<devices>
<device name="" package="SO-08">
<connects>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="INA" pad="2"/>
<connect gate="G$1" pin="INB" pad="3"/>
<connect gate="G$1" pin="OUTA" pad="7"/>
<connect gate="G$1" pin="OUTB" pad="6"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="8"/>
</connects>
<technologies>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7220AD"/>
<attribute name="OC_FARNELL" value="1390649"/>
<attribute name="OC_NEWARK" value="48M0666"/>
</technology>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7220BD"/>
<attribute name="OC_FARNELL" value="1600638"/>
<attribute name="OC_NEWARK" value="94M7887"/>
</technology>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7220CD"/>
<attribute name="OC_FARNELL" value="1390644"/>
<attribute name="OC_NEWARK" value="48M0668"/>
</technology>
<technology name="M">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO7220MD"/>
<attribute name="OC_FARNELL" value="1390646"/>
<attribute name="OC_NEWARK" value="61M6991"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS770*" prefix="IC">
<description>&lt;b&gt;ULTRALOW-POWER 50-mA LOW-DROPOUT LINEAR REGULATORS&lt;/b&gt;&lt;p&gt;
50-mA Low-Dropout Regulator&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps77001.pdf</description>
<gates>
<gate name="G$1" symbol="TPS770XX"/>
</gates>
<devices>
<device name="" package="SOT23-DBV">
<connects>
<connect gate="G$1" pin="!EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="NC/FB" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77001DBVT"/>
<attribute name="OC_FARNELL" value="8461554"/>
<attribute name="OC_NEWARK" value="77C1171"/>
</technology>
<technology name="12">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TPS77012DBVR"/>
<attribute name="OC_FARNELL" value="1412877"/>
<attribute name="OC_NEWARK" value="77C1172"/>
</technology>
<technology name="15">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TPS77015DBVT"/>
<attribute name="OC_FARNELL" value="1412879"/>
<attribute name="OC_NEWARK" value="77C1175"/>
</technology>
<technology name="18">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TPS77018DBVR"/>
<attribute name="OC_FARNELL" value="1575745"/>
<attribute name="OC_NEWARK" value="77C1176"/>
</technology>
<technology name="25">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77025DBVR"/>
<attribute name="OC_FARNELL" value="1412881"/>
<attribute name="OC_NEWARK" value="77C1178"/>
</technology>
<technology name="27">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TPS77027DBVT"/>
<attribute name="OC_FARNELL" value="1510191"/>
<attribute name="OC_NEWARK" value="77C1181"/>
</technology>
<technology name="28">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TPS77028DBVR"/>
<attribute name="OC_FARNELL" value="1412882"/>
<attribute name="OC_NEWARK" value="77C1182"/>
</technology>
<technology name="30">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77030DBVT"/>
<attribute name="OC_FARNELL" value="1207348"/>
<attribute name="OC_NEWARK" value="77C1185"/>
</technology>
<technology name="33">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77033DBVT"/>
<attribute name="OC_FARNELL" value="8461570"/>
<attribute name="OC_NEWARK" value="77C1187"/>
</technology>
<technology name="50">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TPS77050DBVT"/>
<attribute name="OC_FARNELL" value="1412883"/>
<attribute name="OC_NEWARK" value="77C1189"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430FW42*" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
&lt;i&gt;created with make-symbol-device-package-bsdl - text option&lt;/i&gt;&lt;br&gt;
Source: www.ti.com .. MSP430 Microcontroller.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430XW42X"/>
</gates>
<devices>
<device name="IP" package="SQFP-S-10X10-64">
<connects>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="AVSS" pad="62"/>
<connect gate="G$1" pin="COM0" pad="36"/>
<connect gate="G$1" pin="DVCC" pad="1"/>
<connect gate="G$1" pin="DVSS" pad="63"/>
<connect gate="G$1" pin="P1_0/TA0_0" pad="53"/>
<connect gate="G$1" pin="P1_1/TA0_0/MCLK" pad="52"/>
<connect gate="G$1" pin="P1_2/TA0_1" pad="51"/>
<connect gate="G$1" pin="P1_3/TA1_0/SVSOUT" pad="50"/>
<connect gate="G$1" pin="P1_4/TA1_0" pad="49"/>
<connect gate="G$1" pin="P1_5/TA0CLK/ACLK" pad="48"/>
<connect gate="G$1" pin="P1_6/CA0" pad="47"/>
<connect gate="G$1" pin="P1_7/CA1" pad="46"/>
<connect gate="G$1" pin="P2_0/TA0_2" pad="45"/>
<connect gate="G$1" pin="P2_1/TA1_1" pad="44"/>
<connect gate="G$1" pin="P2_2/TA1_2/S23" pad="35"/>
<connect gate="G$1" pin="P2_3/TA1_3/S22" pad="34"/>
<connect gate="G$1" pin="P2_4/TA1_4/S21" pad="33"/>
<connect gate="G$1" pin="P2_5/TA1CLK/S20" pad="32"/>
<connect gate="G$1" pin="P2_6/CAOUT/S19" pad="31"/>
<connect gate="G$1" pin="P2_7/SIFCLKG/S18" pad="30"/>
<connect gate="G$1" pin="P3_0/S17" pad="29"/>
<connect gate="G$1" pin="P3_1/S16" pad="28"/>
<connect gate="G$1" pin="P3_2/S15" pad="27"/>
<connect gate="G$1" pin="P3_3/S14" pad="26"/>
<connect gate="G$1" pin="P3_4/S13" pad="25"/>
<connect gate="G$1" pin="P3_5/S12" pad="24"/>
<connect gate="G$1" pin="P3_6/S11" pad="23"/>
<connect gate="G$1" pin="P3_7/S10" pad="22"/>
<connect gate="G$1" pin="P4_0/S9" pad="21"/>
<connect gate="G$1" pin="P4_1/S8" pad="20"/>
<connect gate="G$1" pin="P4_2/S7" pad="19"/>
<connect gate="G$1" pin="P4_3/S6" pad="18"/>
<connect gate="G$1" pin="P4_4/S5" pad="17"/>
<connect gate="G$1" pin="P4_5/S4" pad="16"/>
<connect gate="G$1" pin="P4_6/S3" pad="15"/>
<connect gate="G$1" pin="P4_7/S2" pad="14"/>
<connect gate="G$1" pin="P5_0/S1" pad="13"/>
<connect gate="G$1" pin="P5_1/S0" pad="12"/>
<connect gate="G$1" pin="P5_2/COM1" pad="37"/>
<connect gate="G$1" pin="P5_3/COM2" pad="38"/>
<connect gate="G$1" pin="P5_4/COM3" pad="39"/>
<connect gate="G$1" pin="P5_5/R13" pad="41"/>
<connect gate="G$1" pin="P5_6/R23" pad="42"/>
<connect gate="G$1" pin="P5_7/R33" pad="43"/>
<connect gate="G$1" pin="P6_0/SIFCH0" pad="59"/>
<connect gate="G$1" pin="P6_1/SIFCH1" pad="60"/>
<connect gate="G$1" pin="P6_2/SIFCH2" pad="61"/>
<connect gate="G$1" pin="P6_3/SIFCH3/SIFCAOUT" pad="2"/>
<connect gate="G$1" pin="P6_4/SIFCI0" pad="3"/>
<connect gate="G$1" pin="P6_5/SIFCI1" pad="4"/>
<connect gate="G$1" pin="P6_6/SIFCI2/SIFDACOUT" pad="5"/>
<connect gate="G$1" pin="P6_7/SIFCI3/SVSIN" pad="6"/>
<connect gate="G$1" pin="R03" pad="40"/>
<connect gate="G$1" pin="RST/NMI" pad="58"/>
<connect gate="G$1" pin="SIFCI" pad="7"/>
<connect gate="G$1" pin="SIFCOM" pad="11"/>
<connect gate="G$1" pin="SIFVSS" pad="10"/>
<connect gate="G$1" pin="TCK" pad="57"/>
<connect gate="G$1" pin="TDI/TCLK" pad="55"/>
<connect gate="G$1" pin="TDO/TDI" pad="54"/>
<connect gate="G$1" pin="TMS" pad="56"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ27010" prefix="IC">
<description>&lt;b&gt;Li-Ion AND Li-Pol BATTERY GAS GAUGE IC FOR PORTABLE APPLICATIONS&lt;/b&gt;&lt;p&gt;
HDQ Communication (bqJUNIOR)&lt;br&gt;
Source: www.ti.com .. bq27010.pdf</description>
<gates>
<gate name="G$1" symbol="BQ27010"/>
<gate name="PP" symbol="PWR-PP10"/>
</gates>
<devices>
<device name="" package="DRK_S-PDSO-N10">
<connects>
<connect gate="G$1" pin="BAT" pad="6"/>
<connect gate="G$1" pin="D/C" pad="4"/>
<connect gate="G$1" pin="GPIO" pad="9"/>
<connect gate="G$1" pin="HDQ" pad="5"/>
<connect gate="G$1" pin="PGM" pad="10"/>
<connect gate="G$1" pin="RBI" pad="1"/>
<connect gate="G$1" pin="SRN" pad="7"/>
<connect gate="G$1" pin="SRP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VSS" pad="3"/>
<connect gate="G$1" pin="VSSG" pad="PP"/>
<connect gate="PP" pin="PP@1" pad="PP@1"/>
<connect gate="PP" pin="PP@10" pad="PP@10"/>
<connect gate="PP" pin="PP@2" pad="PP@2"/>
<connect gate="PP" pin="PP@3" pad="PP@3"/>
<connect gate="PP" pin="PP@4" pad="PP@4"/>
<connect gate="PP" pin="PP@5" pad="PP@5"/>
<connect gate="PP" pin="PP@6" pad="PP@6"/>
<connect gate="PP" pin="PP@7" pad="PP@7"/>
<connect gate="PP" pin="PP@8" pad="PP@8"/>
<connect gate="PP" pin="PP@9" pad="PP@9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ27010DRKR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="02M9376"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ27210" prefix="IC">
<description>&lt;b&gt;Li-Ion AND Li-Pol BATTERY GAS GAUGE IC FOR PORTABLE APPLICATIONS&lt;/b&gt;&lt;p&gt;
I2C  Communication (bqJUNIOR)&lt;br&gt;
Source: www.ti.com .. bq27010.pdf</description>
<gates>
<gate name="PP" symbol="PWR-PP10"/>
<gate name="G$1" symbol="BQ27210"/>
</gates>
<devices>
<device name="" package="DRK_S-PDSO-N10">
<connects>
<connect gate="G$1" pin="BAT" pad="6"/>
<connect gate="G$1" pin="GPIO" pad="9"/>
<connect gate="G$1" pin="PGM" pad="10"/>
<connect gate="G$1" pin="RBI" pad="1"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="5"/>
<connect gate="G$1" pin="SRN" pad="7"/>
<connect gate="G$1" pin="SRP" pad="8"/>
<connect gate="G$1" pin="VCC" pad="2"/>
<connect gate="G$1" pin="VSS" pad="3"/>
<connect gate="G$1" pin="VSSG" pad="PP"/>
<connect gate="PP" pin="PP@1" pad="PP@1"/>
<connect gate="PP" pin="PP@10" pad="PP@10"/>
<connect gate="PP" pin="PP@2" pad="PP@2"/>
<connect gate="PP" pin="PP@3" pad="PP@3"/>
<connect gate="PP" pin="PP@4" pad="PP@4"/>
<connect gate="PP" pin="PP@5" pad="PP@5"/>
<connect gate="PP" pin="PP@6" pad="PP@6"/>
<connect gate="PP" pin="PP@7" pad="PP@7"/>
<connect gate="PP" pin="PP@8" pad="PP@8"/>
<connect gate="PP" pin="PP@9" pad="PP@9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ27210DRKR"/>
<attribute name="OC_FARNELL" value="1534540"/>
<attribute name="OC_NEWARK" value="30M3431"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4041" prefix="IC">
<description>&lt;b&gt;PRECISION MICROPOWER SHUNT VOLTAGE REFERENCE&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slcs146e/slcs146e.pdf</description>
<gates>
<gate name="G$1" symbol="LM4041"/>
</gates>
<devices>
<device name="DBZ" package="DBZ_R-PDSO-G3">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="1"/>
</connects>
<technologies>
<technology name="A12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041A12IDBZR"/>
<attribute name="OC_FARNELL" value="1407949"/>
<attribute name="OC_NEWARK" value="58K5875"/>
</technology>
<technology name="B12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041B12IDBZR"/>
<attribute name="OC_FARNELL" value="1575212"/>
<attribute name="OC_NEWARK" value="58K5882"/>
</technology>
<technology name="C12">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041C12QDBZT"/>
<attribute name="OC_FARNELL" value="1771733"/>
<attribute name="OC_NEWARK" value="43K3376"/>
</technology>
<technology name="D12">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041D12QDBZT"/>
<attribute name="OC_FARNELL" value="1755118"/>
<attribute name="OC_NEWARK" value="43K3381"/>
</technology>
</technologies>
</device>
<device name="DCK" package="DCK_R-PDSO-G5">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="C" pad="3"/>
</connects>
<technologies>
<technology name="A12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041A12IDCKR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="58K5877"/>
</technology>
<technology name="B12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041B12IDCKR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="58K5884"/>
</technology>
<technology name="C12">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041C12IDCKR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="43K3374"/>
</technology>
<technology name="D12">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041D12IDCKR"/>
<attribute name="OC_FARNELL" value="1575129"/>
<attribute name="OC_NEWARK" value="43K3379"/>
</technology>
</technologies>
</device>
<device name="LP" package="LP_O-PBCY-W3">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
</connects>
<technologies>
<technology name="A12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="9486119"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="B12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041C12ILP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M2429"/>
</technology>
<technology name="D12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041D12ILP"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="18M2431"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM4041*I" prefix="IC">
<description>&lt;b&gt;PRECISION MICROPOWER SHUNT VOLTAGE REFERENCE&lt;/b&gt; Adjustable Output&lt;p&gt;
Source: http://focus.ti.com/lit/ds/slcs146e/slcs146e.pdf</description>
<gates>
<gate name="G$1" symbol="LM4041-ADJ"/>
</gates>
<devices>
<device name="DBZ" package="DBZ_R-PDSO-G3">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="FB" pad="1"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041CIDBZR"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="31K7136"/>
</technology>
<technology name="D">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041DIDBZR"/>
<attribute name="OC_FARNELL" value="1053788"/>
<attribute name="OC_NEWARK" value="31K7146"/>
</technology>
</technologies>
</device>
<device name="DCK" package="DCK_R-PDSO-G5">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="3"/>
<connect gate="G$1" pin="FB" pad="5"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041BIDCKRG4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="41M3455"/>
</technology>
<technology name="C">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041CIDCKR"/>
<attribute name="OC_FARNELL" value="1053797"/>
<attribute name="OC_NEWARK" value="31K7140"/>
</technology>
<technology name="D">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="LM4041DIDCKR"/>
<attribute name="OC_FARNELL" value="1053783"/>
<attribute name="OC_NEWARK" value="31K7150"/>
</technology>
</technologies>
</device>
<device name="LP" package="LP_O-PBCY-W3">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="FB" pad="1"/>
</connects>
<technologies>
<technology name="B">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041CILP"/>
<attribute name="OC_FARNELL" value="1673945"/>
<attribute name="OC_NEWARK" value="50M8856"/>
</technology>
<technology name="D">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LM4041DILP"/>
<attribute name="OC_FARNELL" value="9486119"/>
<attribute name="OC_NEWARK" value="50M8858"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430F54*" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 27&lt;/i&gt;&lt;br&gt;
Source: www.ti.com .. msp430f5437.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430F5437-100"/>
</gates>
<devices>
<device name="" package="PZ_S-PQFP-G100">
<connects>
<connect gate="G$1" pin="AVCC" pad="11"/>
<connect gate="G$1" pin="AVSS" pad="12"/>
<connect gate="G$1" pin="DVCC1" pad="16"/>
<connect gate="G$1" pin="DVCC2" pad="64"/>
<connect gate="G$1" pin="DVCC3" pad="38"/>
<connect gate="G$1" pin="DVCC4" pad="87"/>
<connect gate="G$1" pin="DVSS1" pad="15"/>
<connect gate="G$1" pin="DVSS2" pad="63"/>
<connect gate="G$1" pin="DVSS3" pad="37"/>
<connect gate="G$1" pin="DVSS4" pad="88"/>
<connect gate="G$1" pin="P10_0/UCB3STE/UCA3CLK" pad="76"/>
<connect gate="G$1" pin="P10_1/UCB3SIMO/UCB3SDA" pad="77"/>
<connect gate="G$1" pin="P10_2/UCB3SOMI/UCB3SCL" pad="78"/>
<connect gate="G$1" pin="P10_3/UCB3CLK/UCA3STE" pad="79"/>
<connect gate="G$1" pin="P10_4/UCA3TXD/UCA3SIMO" pad="80"/>
<connect gate="G$1" pin="P10_5/UCA3RXD/UCA3SOMI" pad="81"/>
<connect gate="G$1" pin="P10_6" pad="82"/>
<connect gate="G$1" pin="P10_7" pad="83"/>
<connect gate="G$1" pin="P11_0/ACLK" pad="84"/>
<connect gate="G$1" pin="P11_1/MCLK" pad="85"/>
<connect gate="G$1" pin="P11_2/SMCLK" pad="86"/>
<connect gate="G$1" pin="P1_0/TA0CLK/ACLK" pad="17"/>
<connect gate="G$1" pin="P1_1/TA0.0" pad="18"/>
<connect gate="G$1" pin="P1_2/TA0.1" pad="19"/>
<connect gate="G$1" pin="P1_3/TA0.2" pad="20"/>
<connect gate="G$1" pin="P1_4/TA0.3" pad="21"/>
<connect gate="G$1" pin="P1_5/TA0.4" pad="22"/>
<connect gate="G$1" pin="P1_6/SMCLK" pad="23"/>
<connect gate="G$1" pin="P1_7" pad="24"/>
<connect gate="G$1" pin="P2_0/TA1CLK/MCLK" pad="25"/>
<connect gate="G$1" pin="P2_1/TA1.0" pad="26"/>
<connect gate="G$1" pin="P2_2/TA1.1" pad="27"/>
<connect gate="G$1" pin="P2_3/TA1.2" pad="28"/>
<connect gate="G$1" pin="P2_4/RTCCLK" pad="29"/>
<connect gate="G$1" pin="P2_5" pad="30"/>
<connect gate="G$1" pin="P2_6/ACLK" pad="31"/>
<connect gate="G$1" pin="P2_7/ADC12CLK/DMAE0" pad="32"/>
<connect gate="G$1" pin="P3_0/UCB0STE/UCA0CLK" pad="33"/>
<connect gate="G$1" pin="P3_1/UCB0SIMO/UCB0SDA" pad="34"/>
<connect gate="G$1" pin="P3_2/UCB0SOMI/UCB0SCL" pad="35"/>
<connect gate="G$1" pin="P3_3/UCB0CLK/UCA0STE" pad="36"/>
<connect gate="G$1" pin="P3_4/UCA0TXD/UCA0SIMO" pad="39"/>
<connect gate="G$1" pin="P3_5/UCA0RXD/UCA0SOMI" pad="40"/>
<connect gate="G$1" pin="P3_6/UCB1STE/UCA1CLK" pad="41"/>
<connect gate="G$1" pin="P3_7/UCB1SIMO/UCB1SDA" pad="42"/>
<connect gate="G$1" pin="P4_0/TB0" pad="43"/>
<connect gate="G$1" pin="P4_1/TB1" pad="44"/>
<connect gate="G$1" pin="P4_2/TB2" pad="45"/>
<connect gate="G$1" pin="P4_3/TB3" pad="46"/>
<connect gate="G$1" pin="P4_4/TB4" pad="47"/>
<connect gate="G$1" pin="P4_5/TB5" pad="48"/>
<connect gate="G$1" pin="P4_6/TB6" pad="49"/>
<connect gate="G$1" pin="P4_7/TBCLK/SMCLK" pad="50"/>
<connect gate="G$1" pin="P5_0/VREF+/VEREF+" pad="9"/>
<connect gate="G$1" pin="P5_1/VREF-/VEREF-" pad="10"/>
<connect gate="G$1" pin="P5_2/XT2IN" pad="89"/>
<connect gate="G$1" pin="P5_3/XT2OUT" pad="90"/>
<connect gate="G$1" pin="P5_4/UCB1SOMI/UCB1SCL" pad="51"/>
<connect gate="G$1" pin="P5_5/UCB1CLK/UCA1STE" pad="52"/>
<connect gate="G$1" pin="P5_6/UCA1TXD/UCA1SIMO" pad="53"/>
<connect gate="G$1" pin="P5_7/UCA1RXD/UCA1SOMI" pad="54"/>
<connect gate="G$1" pin="P6_0/A0" pad="97"/>
<connect gate="G$1" pin="P6_1/A1" pad="98"/>
<connect gate="G$1" pin="P6_2/A2" pad="99"/>
<connect gate="G$1" pin="P6_3/A3" pad="100"/>
<connect gate="G$1" pin="P6_4/A4" pad="1"/>
<connect gate="G$1" pin="P6_5/A5" pad="2"/>
<connect gate="G$1" pin="P6_6/A6" pad="3"/>
<connect gate="G$1" pin="P6_7/A7" pad="4"/>
<connect gate="G$1" pin="P7_0/XIN" pad="13"/>
<connect gate="G$1" pin="P7_1/XOUT" pad="14"/>
<connect gate="G$1" pin="P7_2/TBOUTH/SVMOUT" pad="55"/>
<connect gate="G$1" pin="P7_3/TA1.2" pad="56"/>
<connect gate="G$1" pin="P7_4/A12" pad="5"/>
<connect gate="G$1" pin="P7_5/A13" pad="6"/>
<connect gate="G$1" pin="P7_6/A14" pad="7"/>
<connect gate="G$1" pin="P7_7/A15" pad="8"/>
<connect gate="G$1" pin="P8_0/TA0.0" pad="57"/>
<connect gate="G$1" pin="P8_1/TA0.1" pad="58"/>
<connect gate="G$1" pin="P8_2/TA0.2" pad="59"/>
<connect gate="G$1" pin="P8_3/TA0.3" pad="60"/>
<connect gate="G$1" pin="P8_4/TA0.4" pad="61"/>
<connect gate="G$1" pin="P8_5/TA1.0" pad="65"/>
<connect gate="G$1" pin="P8_6/TA1.1" pad="66"/>
<connect gate="G$1" pin="P8_7" pad="67"/>
<connect gate="G$1" pin="P9_0/UCB2STE/UCA2CLK" pad="68"/>
<connect gate="G$1" pin="P9_1/UCB2SIMO/UCB2SDA" pad="69"/>
<connect gate="G$1" pin="P9_2/UCB2SOMI/UCB2SCL" pad="70"/>
<connect gate="G$1" pin="P9_3/UCB2CLK/UCA2STE" pad="71"/>
<connect gate="G$1" pin="P9_4/UCA2TXD/UCA2SIMO" pad="72"/>
<connect gate="G$1" pin="P9_5/UCA2RXD/UCA2SOMI" pad="73"/>
<connect gate="G$1" pin="P9_6" pad="74"/>
<connect gate="G$1" pin="P9_7" pad="75"/>
<connect gate="G$1" pin="PJ_0/TDO" pad="92"/>
<connect gate="G$1" pin="PJ_1/TDI/TCLK" pad="93"/>
<connect gate="G$1" pin="PJ_2/TMS" pad="94"/>
<connect gate="G$1" pin="PJ_3/TCK" pad="95"/>
<connect gate="G$1" pin="RST/NMI/SBWTDIO" pad="96"/>
<connect gate="G$1" pin="TEST/SBWTCK" pad="91"/>
<connect gate="G$1" pin="VCORE" pad="62"/>
</connects>
<technologies>
<technology name="19">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5419IPZR"/>
<attribute name="OC_FARNELL" value="1740335"/>
<attribute name="OC_NEWARK" value="12P7733"/>
</technology>
<technology name="19A">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="36">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5436IPZ"/>
<attribute name="OC_FARNELL" value="1740338"/>
<attribute name="OC_NEWARK" value="86R1301"/>
</technology>
<technology name="36A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5436AIPZ"/>
<attribute name="OC_FARNELL" value="1740338"/>
<attribute name="OC_NEWARK" value="68R9298"/>
</technology>
<technology name="38">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5438IPZ"/>
<attribute name="OC_FARNELL" value="1740340"/>
<attribute name="OC_NEWARK" value="77R3126"/>
</technology>
<technology name="38A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5438AIPZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="68R9304"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430F5*" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 27&lt;/i&gt;&lt;br&gt;
Source: www.ti.com .. msp430f5437.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430F5437-80"/>
</gates>
<devices>
<device name="" package="PN_S-PQFP-G80">
<connects>
<connect gate="G$1" pin="!RST!/NMI/SBWTDIO" pad="76"/>
<connect gate="G$1" pin="AVCC" pad="11"/>
<connect gate="G$1" pin="AVSS" pad="12"/>
<connect gate="G$1" pin="DVCC1" pad="16"/>
<connect gate="G$1" pin="DVCC2" pad="51"/>
<connect gate="G$1" pin="DVCC3" pad="31"/>
<connect gate="G$1" pin="DVCC4" pad="67"/>
<connect gate="G$1" pin="DVSS1" pad="15"/>
<connect gate="G$1" pin="DVSS2" pad="50"/>
<connect gate="G$1" pin="DVSS3" pad="30"/>
<connect gate="G$1" pin="DVSS4" pad="68"/>
<connect gate="G$1" pin="P1_0/TA0CLK/ACLK" pad="17"/>
<connect gate="G$1" pin="P1_1/TA0.0" pad="18"/>
<connect gate="G$1" pin="P1_2/TA0.1" pad="19"/>
<connect gate="G$1" pin="P1_3/TA0.2" pad="20"/>
<connect gate="G$1" pin="P1_4/TA0.3" pad="21"/>
<connect gate="G$1" pin="P1_5/TA0.4" pad="22"/>
<connect gate="G$1" pin="P1_6/SMCLK" pad="23"/>
<connect gate="G$1" pin="P1_7" pad="24"/>
<connect gate="G$1" pin="P2_0/TA1CLK/MCLK" pad="25"/>
<connect gate="G$1" pin="P2_1/TA1.0" pad="26"/>
<connect gate="G$1" pin="P2_2/TA1.1" pad="27"/>
<connect gate="G$1" pin="P2_3/TA1.2" pad="28"/>
<connect gate="G$1" pin="P2_4/RTCCLK" pad="29"/>
<connect gate="G$1" pin="P2_5" pad="32"/>
<connect gate="G$1" pin="P2_6/ACLK" pad="33"/>
<connect gate="G$1" pin="P2_7/ADC12CLK/DMAE0" pad="34"/>
<connect gate="G$1" pin="P3_0/UCB0STE/UCA0CLK" pad="35"/>
<connect gate="G$1" pin="P3_1/UCB0SIMO/UCB0SDA" pad="36"/>
<connect gate="G$1" pin="P3_2/UCB0SOMI/UCB0SCL" pad="37"/>
<connect gate="G$1" pin="P3_3/UCB0CLK/UCA0STE" pad="38"/>
<connect gate="G$1" pin="P3_4/UCA0TXD/UCA0SIMO" pad="39"/>
<connect gate="G$1" pin="P3_5/UCA0RXD/UCA0SOMI" pad="40"/>
<connect gate="G$1" pin="P3_6/UCB1STE/UCA1CLK" pad="41"/>
<connect gate="G$1" pin="P3_7/UCB1SIMO/UCB1SDA" pad="42"/>
<connect gate="G$1" pin="P4_0/TB0" pad="43"/>
<connect gate="G$1" pin="P4_1/TB1" pad="44"/>
<connect gate="G$1" pin="P4_2/TB2" pad="45"/>
<connect gate="G$1" pin="P4_3/TB3" pad="46"/>
<connect gate="G$1" pin="P4_4/TB4" pad="47"/>
<connect gate="G$1" pin="P4_5/TB5" pad="48"/>
<connect gate="G$1" pin="P4_6/TB6" pad="52"/>
<connect gate="G$1" pin="P4_7/TBCLK/SMCLK" pad="53"/>
<connect gate="G$1" pin="P5_0/VREF+/VEREF+" pad="9"/>
<connect gate="G$1" pin="P5_1/VREF-/VEREF-" pad="10"/>
<connect gate="G$1" pin="P5_2/XT2IN" pad="69"/>
<connect gate="G$1" pin="P5_3/XT2OUT" pad="70"/>
<connect gate="G$1" pin="P5_4/UCB1SOMI/UCB1SCL" pad="54"/>
<connect gate="G$1" pin="P5_5/UCB1CLK/UCA1STE" pad="55"/>
<connect gate="G$1" pin="P5_6/UCA1TXD/UCA1SIMO" pad="56"/>
<connect gate="G$1" pin="P5_7/UCA1RXD/UCA1SOMI" pad="57"/>
<connect gate="G$1" pin="P6_0/A0" pad="77"/>
<connect gate="G$1" pin="P6_1/A1" pad="78"/>
<connect gate="G$1" pin="P6_2/A2" pad="79"/>
<connect gate="G$1" pin="P6_3/A3" pad="80"/>
<connect gate="G$1" pin="P6_4/A4" pad="1"/>
<connect gate="G$1" pin="P6_5/A5" pad="2"/>
<connect gate="G$1" pin="P6_6/A6" pad="3"/>
<connect gate="G$1" pin="P6_7/A7" pad="4"/>
<connect gate="G$1" pin="P7_0/XIN" pad="13"/>
<connect gate="G$1" pin="P7_1/XOUT" pad="14"/>
<connect gate="G$1" pin="P7_2/TBOUTH/SVMOUT" pad="58"/>
<connect gate="G$1" pin="P7_3/TA1.2" pad="59"/>
<connect gate="G$1" pin="P7_4/A12" pad="5"/>
<connect gate="G$1" pin="P7_5/A13" pad="6"/>
<connect gate="G$1" pin="P7_6/A14" pad="7"/>
<connect gate="G$1" pin="P7_7/A15" pad="8"/>
<connect gate="G$1" pin="P8_0/TA0.0" pad="60"/>
<connect gate="G$1" pin="P8_1/TA0.1" pad="61"/>
<connect gate="G$1" pin="P8_2/TA0.2" pad="62"/>
<connect gate="G$1" pin="P8_3/TA0.3" pad="63"/>
<connect gate="G$1" pin="P8_4/TA0.4" pad="64"/>
<connect gate="G$1" pin="P8_5/TA1.0" pad="65"/>
<connect gate="G$1" pin="P8_6/TA1.1" pad="66"/>
<connect gate="G$1" pin="PJ_0/TDO" pad="72"/>
<connect gate="G$1" pin="PJ_1/TDI/TCLK" pad="73"/>
<connect gate="G$1" pin="PJ_2/TMS" pad="74"/>
<connect gate="G$1" pin="PJ_3/TCK" pad="75"/>
<connect gate="G$1" pin="TEST/SBWTCK" pad="71"/>
<connect gate="G$1" pin="VCORE" pad="49"/>
</connects>
<technologies>
<technology name="418">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5418IPN"/>
<attribute name="OC_FARNELL" value="1740334"/>
<attribute name="OC_NEWARK" value="84R7421"/>
</technology>
<technology name="418A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5418AIPN"/>
<attribute name="OC_FARNELL" value="1740334"/>
<attribute name="OC_NEWARK" value="68R9290"/>
</technology>
<technology name="435">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5435AIPN"/>
<attribute name="OC_FARNELL" value="1740336"/>
<attribute name="OC_NEWARK" value="68R9296"/>
</technology>
<technology name="435A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5435AIPN"/>
<attribute name="OC_FARNELL" value="1740336"/>
<attribute name="OC_NEWARK" value="68R9296"/>
</technology>
<technology name="437">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5437IPN"/>
<attribute name="OC_FARNELL" value="1740339"/>
<attribute name="OC_NEWARK" value="87R0103"/>
</technology>
<technology name="437A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F5437AIPN"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="68R9302"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430F22*2IDA" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;
Source: http://focus.ti.com/lit/ds/symlink/msp430f2274.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430X22X2-DA"/>
</gates>
<devices>
<device name="" package="TSSOP38_R-PDSO-G38-DA">
<connects>
<connect gate="G$1" pin="!RST!/NMI/SBWTDIO" pad="7"/>
<connect gate="G$1" pin="AVCC" pad="16"/>
<connect gate="G$1" pin="AVSS" pad="15"/>
<connect gate="G$1" pin="DVCC" pad="2"/>
<connect gate="G$1" pin="DVSS" pad="4"/>
<connect gate="G$1" pin="P1.0/TACLK/ADC10CLK" pad="31"/>
<connect gate="G$1" pin="P1.1/TA0" pad="32"/>
<connect gate="G$1" pin="P1.2/TA1" pad="33"/>
<connect gate="G$1" pin="P1.3/TA2" pad="34"/>
<connect gate="G$1" pin="P1.4/SMCLK/TCK" pad="35"/>
<connect gate="G$1" pin="P1.5/TA0/TMS" pad="36"/>
<connect gate="G$1" pin="P1.6/TA1/TDI/TCLK" pad="37"/>
<connect gate="G$1" pin="P1.7/TA2/TDO/TDI" pad="38"/>
<connect gate="G$1" pin="P2.0/ACLK/A0" pad="8"/>
<connect gate="G$1" pin="P2.1/TAINCLK/SMCLK/A1" pad="9"/>
<connect gate="G$1" pin="P2.2/TA0/A2" pad="10"/>
<connect gate="G$1" pin="P2.3/TA1/A3/VREF-/VEREF-" pad="29"/>
<connect gate="G$1" pin="P2.4/TA2/A4/VREF+/VEREF+" pad="30"/>
<connect gate="G$1" pin="P2.5/ROSC" pad="3"/>
<connect gate="G$1" pin="P3.0/UCB0STE/UCA0CLK/A5" pad="11"/>
<connect gate="G$1" pin="P3.1/UCB0SIMO/UCB0SDA" pad="12"/>
<connect gate="G$1" pin="P3.2/UCB0SOMI/UCB0SCL" pad="13"/>
<connect gate="G$1" pin="P3.3/UCB0CLK/UCA0STE" pad="14"/>
<connect gate="G$1" pin="P3.4/UCA0TXD/UCA0SIMO" pad="25"/>
<connect gate="G$1" pin="P3.5/UCA0RXD/UCA0SOMI" pad="26"/>
<connect gate="G$1" pin="P3.6/A6" pad="27"/>
<connect gate="G$1" pin="P3.7/A7" pad="28"/>
<connect gate="G$1" pin="P4.0/TB0" pad="17"/>
<connect gate="G$1" pin="P4.1/TB1" pad="18"/>
<connect gate="G$1" pin="P4.2/TB2" pad="19"/>
<connect gate="G$1" pin="P4.3/TB0/A12" pad="20"/>
<connect gate="G$1" pin="P4.4/TB1A13" pad="21"/>
<connect gate="G$1" pin="P4.5/TB2A14" pad="22"/>
<connect gate="G$1" pin="P4.6/TBOUTHA15" pad="23"/>
<connect gate="G$1" pin="P4.7/TBCLK" pad="24"/>
<connect gate="G$1" pin="TEST/SBWTCK" pad="1"/>
<connect gate="G$1" pin="XIN/P2.6" pad="6"/>
<connect gate="G$1" pin="XOUT/P2.7" pad="5"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F2232IDA"/>
<attribute name="OC_FARNELL" value="1610178"/>
<attribute name="OC_NEWARK" value="28M6312"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F2252IDA"/>
<attribute name="OC_FARNELL" value="1649421"/>
<attribute name="OC_NEWARK" value="28M6328"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F2272IDA"/>
<attribute name="OC_FARNELL" value="1537188"/>
<attribute name="OC_NEWARK" value="95M6767"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430F22*4IDA" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;
Source: http://focus.ti.com/lit/ds/symlink/msp430f2274.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430X22X4-DA"/>
</gates>
<devices>
<device name="" package="TSSOP38_R-PDSO-G38-DA">
<connects>
<connect gate="G$1" pin="!RST!/NMI/SBWTDIO" pad="7"/>
<connect gate="G$1" pin="AVCC" pad="16"/>
<connect gate="G$1" pin="AVSS" pad="15"/>
<connect gate="G$1" pin="DVCC" pad="2"/>
<connect gate="G$1" pin="DVSS" pad="4"/>
<connect gate="G$1" pin="P1.0/TACLK/ADC10CLK" pad="31"/>
<connect gate="G$1" pin="P1.1/TA0" pad="32"/>
<connect gate="G$1" pin="P1.2/TA1" pad="33"/>
<connect gate="G$1" pin="P1.3/TA2" pad="34"/>
<connect gate="G$1" pin="P1.4/SMCLK/TCK" pad="35"/>
<connect gate="G$1" pin="P1.5/TA0/TMS" pad="36"/>
<connect gate="G$1" pin="P1.6/TA1/TDI/TCLK" pad="37"/>
<connect gate="G$1" pin="P1.7/TA2/TDO/TDI" pad="38"/>
<connect gate="G$1" pin="P2.0/ACLK/A0/OA0I0" pad="8"/>
<connect gate="G$1" pin="P2.1/TAINCLK/SMCLK/A1/OA0O" pad="9"/>
<connect gate="G$1" pin="P2.2/TA0/A2/OA0I1" pad="10"/>
<connect gate="G$1" pin="P2.3/TA1/A3/VREF-/VEREF-/OA1I1/OA1O" pad="29"/>
<connect gate="G$1" pin="P2.4/TA2/A4/VREF+/VEREF+/OA1I0" pad="30"/>
<connect gate="G$1" pin="P2.5/ROSC" pad="3"/>
<connect gate="G$1" pin="P3.0/UCB0STE/UCA0CLK/A5" pad="11"/>
<connect gate="G$1" pin="P3.1/UCB0SIMO/UCB0SDA" pad="12"/>
<connect gate="G$1" pin="P3.2/UCB0SOMI/UCB0SCL" pad="13"/>
<connect gate="G$1" pin="P3.3/UCB0CLK/UCA0STE" pad="14"/>
<connect gate="G$1" pin="P3.4/UCA0TXD/UCA0SIMO" pad="25"/>
<connect gate="G$1" pin="P3.5/UCA0RXD/UCA0SOMI" pad="26"/>
<connect gate="G$1" pin="P3.6/A6/OA0I2" pad="27"/>
<connect gate="G$1" pin="P3.7/A7/OA1I2" pad="28"/>
<connect gate="G$1" pin="P4.0/TB0" pad="17"/>
<connect gate="G$1" pin="P4.1/TB1" pad="18"/>
<connect gate="G$1" pin="P4.2/TB2" pad="19"/>
<connect gate="G$1" pin="P4.3/TB0/A12/OA0O" pad="20"/>
<connect gate="G$1" pin="P4.4/TB1A13/OA1O" pad="21"/>
<connect gate="G$1" pin="P4.5/TB2A14/OA0I3" pad="22"/>
<connect gate="G$1" pin="P4.6/TBOUTHA15/OA1I3" pad="23"/>
<connect gate="G$1" pin="P4.7/TBCLK" pad="24"/>
<connect gate="G$1" pin="TEST/SBWTCK" pad="1"/>
<connect gate="G$1" pin="XIN/P2.6" pad="6"/>
<connect gate="G$1" pin="XOUT/P2.7" pad="5"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F2234IDA"/>
<attribute name="OC_FARNELL" value="1649419"/>
<attribute name="OC_NEWARK" value="28M6320"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F2254IDA"/>
<attribute name="OC_FARNELL" value="1649422"/>
<attribute name="OC_NEWARK" value="28M6334"/>
</technology>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F2274IDA"/>
<attribute name="OC_FARNELL" value="1610179"/>
<attribute name="OC_NEWARK" value="28M6350"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS773*" prefix="IC">
<description>&lt;B&gt;250-mA LDO REGULATORS WITH RESET OUTPUT&lt;/b&gt;&lt;p&gt;

&lt;p&gt; Source: &lt;a href="http://www.ti.com/lit/ds/symlink/tps773.pdf"&gt;(TPS773)&lt;/a&gt;

&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="TPS773XX"/>
</gates>
<devices>
<device name="" package="DGK_S-PDSO-G8">
<connects>
<connect gate="G$1" pin="!EN" pad="3"/>
<connect gate="G$1" pin="!RESET" pad="2"/>
<connect gate="G$1" pin="FB/SENSE" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN@1" pad="5"/>
<connect gate="G$1" pin="IN@2" pad="6"/>
<connect gate="G$1" pin="OUT@1" pad="7"/>
<connect gate="G$1" pin="OUT@2" pad="8"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77301DGK"/>
<attribute name="OC_FARNELL" value="1510194"/>
<attribute name="OC_NEWARK" value="77C1213"/>
</technology>
<technology name="15">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77315DGK"/>
<attribute name="OC_FARNELL" value="1412890"/>
<attribute name="OC_NEWARK" value="77C1215"/>
</technology>
<technology name="16">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77316DGK"/>
<attribute name="OC_FARNELL" value="1412891"/>
<attribute name="OC_NEWARK" value="77C1217"/>
</technology>
<technology name="18">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77318DGK"/>
<attribute name="OC_FARNELL" value="1412893"/>
<attribute name="OC_NEWARK" value="77C1219"/>
</technology>
<technology name="27">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77327DGK"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="77C1221"/>
</technology>
<technology name="28">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77328DGK"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="77C1223"/>
</technology>
<technology name="33">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77333DGK"/>
<attribute name="OC_FARNELL" value="1510195"/>
<attribute name="OC_NEWARK" value="02M1919"/>
</technology>
<technology name="50">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TPS77350DGK"/>
<attribute name="OC_FARNELL" value="1412894"/>
<attribute name="OC_NEWARK" value="77C1226"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS774*" prefix="IC">
<description>&lt;B&gt;250-mA LDO REGULATORS WITH POWER GOOD OUTPUT&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/tps773.pdf"&gt;(TPS774)&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TPS774XX"/>
</gates>
<devices>
<device name="" package="DGK_S-PDSO-G8">
<connects>
<connect gate="G$1" pin="!EN" pad="3"/>
<connect gate="G$1" pin="FB/SENSE" pad="1"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN@1" pad="5"/>
<connect gate="G$1" pin="IN@2" pad="6"/>
<connect gate="G$1" pin="OUT@1" pad="7"/>
<connect gate="G$1" pin="OUT@2" pad="8"/>
<connect gate="G$1" pin="PG" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1412896"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6300*" prefix="IC">
<description>&lt;b&gt;HIGH EFFICIENT SINGLE INDUCTOR BUCK-BOOST CONVERTER WITH 1.8-A SWITCHES&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tps63001.pdf</description>
<gates>
<gate name="G$1" symbol="TPS6300X"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="DRC-S-PVSON-N10">
<connects>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="FB" pad="10"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="L1" pad="4"/>
<connect gate="G$1" pin="L2" pad="2"/>
<connect gate="G$1" pin="PGND" pad="3"/>
<connect gate="G$1" pin="PS/SYNC" pad="7"/>
<connect gate="G$1" pin="VIN" pad="5"/>
<connect gate="G$1" pin="VINA" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="1"/>
<connect gate="TH" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS63000DRCTG4"/>
<attribute name="OC_FARNELL" value="1511852"/>
<attribute name="OC_NEWARK" value="59M7217"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC*637" prefix="IC">
<description>&lt;b&gt;Switched Mode Controller for DC Motor Drive&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/uc3637.pdf</description>
<gates>
<gate name="G$1" symbol="UC3637N"/>
</gates>
<devices>
<device name="N" package="DIL18">
<connects>
<connect gate="G$1" pin="+AIN" pad="11"/>
<connect gate="G$1" pin="+BIN" pad="8"/>
<connect gate="G$1" pin="+C/L" pad="12"/>
<connect gate="G$1" pin="+E/A" pad="15"/>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="+VTH" pad="1"/>
<connect gate="G$1" pin="-AIN" pad="10"/>
<connect gate="G$1" pin="-BIN" pad="9"/>
<connect gate="G$1" pin="-C/L" pad="13"/>
<connect gate="G$1" pin="-E/A" pad="16"/>
<connect gate="G$1" pin="-VS" pad="5"/>
<connect gate="G$1" pin="-VTH" pad="3"/>
<connect gate="G$1" pin="AOUT" pad="4"/>
<connect gate="G$1" pin="BOUT" pad="7"/>
<connect gate="G$1" pin="CT" pad="2"/>
<connect gate="G$1" pin="E/A_OUT" pad="17"/>
<connect gate="G$1" pin="ISET" pad="18"/>
<connect gate="G$1" pin="SH_DOWN" pad="14"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC2637N"/>
<attribute name="OC_FARNELL" value="1207367"/>
<attribute name="OC_NEWARK" value="77C2829"/>
</technology>
<technology name="3">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC3637N"/>
<attribute name="OC_FARNELL" value="1107292"/>
<attribute name="OC_NEWARK" value="62K3473"/>
</technology>
</technologies>
</device>
<device name="DW" package="SO-20DW">
<connects>
<connect gate="G$1" pin="+AIN" pad="13"/>
<connect gate="G$1" pin="+BIN" pad="8"/>
<connect gate="G$1" pin="+C/L" pad="14"/>
<connect gate="G$1" pin="+E/A" pad="17"/>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="+VTH" pad="1"/>
<connect gate="G$1" pin="-AIN" pad="12"/>
<connect gate="G$1" pin="-BIN" pad="9"/>
<connect gate="G$1" pin="-C/L" pad="15"/>
<connect gate="G$1" pin="-E/A" pad="18"/>
<connect gate="G$1" pin="-VS" pad="5"/>
<connect gate="G$1" pin="-VTH" pad="3"/>
<connect gate="G$1" pin="AOUT" pad="4"/>
<connect gate="G$1" pin="BOUT" pad="7"/>
<connect gate="G$1" pin="CT" pad="2"/>
<connect gate="G$1" pin="E/A_OUT" pad="19"/>
<connect gate="G$1" pin="ISET" pad="20"/>
<connect gate="G$1" pin="SH_DOWN" pad="16"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC2637DW"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="77C2827"/>
</technology>
<technology name="3">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC3637DW"/>
<attribute name="OC_FARNELL" value="1212378"/>
<attribute name="OC_NEWARK" value="77C3168"/>
</technology>
</technologies>
</device>
<device name="Q" package="PLCC20">
<connects>
<connect gate="G$1" pin="+AIN" pad="12"/>
<connect gate="G$1" pin="+BIN" pad="9"/>
<connect gate="G$1" pin="+C/L" pad="13"/>
<connect gate="G$1" pin="+E/A" pad="17"/>
<connect gate="G$1" pin="+VS" pad="7"/>
<connect gate="G$1" pin="+VTH" pad="1"/>
<connect gate="G$1" pin="-AIN" pad="11"/>
<connect gate="G$1" pin="-BIN" pad="10"/>
<connect gate="G$1" pin="-C/L" pad="14"/>
<connect gate="G$1" pin="-E/A" pad="18"/>
<connect gate="G$1" pin="-VS" pad="5"/>
<connect gate="G$1" pin="-VTH" pad="3"/>
<connect gate="G$1" pin="AOUT" pad="4"/>
<connect gate="G$1" pin="BOUT" pad="8"/>
<connect gate="G$1" pin="CT" pad="2"/>
<connect gate="G$1" pin="E/A_OUT" pad="19"/>
<connect gate="G$1" pin="ISET" pad="20"/>
<connect gate="G$1" pin="SH_DOWN" pad="15"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="UC2637Q"/>
<attribute name="OC_FARNELL" value="1510339"/>
<attribute name="OC_NEWARK" value="77C2830"/>
</technology>
<technology name="3">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="UC3637Q"/>
<attribute name="OC_FARNELL" value="1413281"/>
<attribute name="OC_NEWARK" value="05C3766"/>
</technology>
</technologies>
</device>
<device name="J" package="DIL18">
<connects>
<connect gate="G$1" pin="+AIN" pad="11"/>
<connect gate="G$1" pin="+BIN" pad="8"/>
<connect gate="G$1" pin="+C/L" pad="12"/>
<connect gate="G$1" pin="+E/A" pad="15"/>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="+VTH" pad="1"/>
<connect gate="G$1" pin="-AIN" pad="10"/>
<connect gate="G$1" pin="-BIN" pad="9"/>
<connect gate="G$1" pin="-C/L" pad="13"/>
<connect gate="G$1" pin="-E/A" pad="16"/>
<connect gate="G$1" pin="-VS" pad="5"/>
<connect gate="G$1" pin="-VTH" pad="3"/>
<connect gate="G$1" pin="AOUT" pad="4"/>
<connect gate="G$1" pin="BOUT" pad="7"/>
<connect gate="G$1" pin="CT" pad="2"/>
<connect gate="G$1" pin="E/A_OUT" pad="17"/>
<connect gate="G$1" pin="ISET" pad="18"/>
<connect gate="G$1" pin="SH_DOWN" pad="14"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPA6132A2" prefix="IC">
<description>&lt;b&gt;25-mW DIRECTPATH (TM) STEREO HEADPHONE AMPLIFIER WITH POP SUPPRESSION&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. tpa6132a2 direct path stereo $.65.pdf</description>
<gates>
<gate name="G$1" symbol="TPA6132A2"/>
</gates>
<devices>
<device name="" package="QFN16">
<connects>
<connect gate="G$1" pin="CPN" pad="9"/>
<connect gate="G$1" pin="CPP" pad="11"/>
<connect gate="G$1" pin="EN" pad="13"/>
<connect gate="G$1" pin="G1" pad="7"/>
<connect gate="G$1" pin="GO" pad="6"/>
<connect gate="G$1" pin="HPVDD" pad="12"/>
<connect gate="G$1" pin="HPVSS" pad="8"/>
<connect gate="G$1" pin="INL+" pad="2"/>
<connect gate="G$1" pin="INL-" pad="1"/>
<connect gate="G$1" pin="INR+" pad="3"/>
<connect gate="G$1" pin="INR-" pad="4"/>
<connect gate="G$1" pin="OUTL" pad="16"/>
<connect gate="G$1" pin="OUTR" pad="5"/>
<connect gate="G$1" pin="PGND" pad="10"/>
<connect gate="G$1" pin="SGND" pad="15"/>
<connect gate="G$1" pin="TH" pad="TH"/>
<connect gate="G$1" pin="VDD" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPA6132A2RTET"/>
<attribute name="OC_FARNELL" value="1697167"/>
<attribute name="OC_NEWARK" value="46P3781"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPA3123D2" prefix="IC">
<description>&lt;b&gt;25-W STEREO CLASS-D AUDIO POWER AMPLIFIER&lt;/b&gt;&lt;p&gt;
&lt;font color="red"&gt;Please INVOKE gate EXP, set DRC-Clearance | Same signals | SMD - SMD = 0&lt;/font&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tpa3123d2.pdf</description>
<gates>
<gate name="G$1" symbol="TPA3123D2"/>
<gate name="EXP" symbol="EXP19"/>
</gates>
<devices>
<device name="" package="PWP-TSSOP24">
<connects>
<connect gate="EXP" pin="EXP" pad="EXP"/>
<connect gate="EXP" pin="EXP@1" pad="EXP@1"/>
<connect gate="EXP" pin="EXP@10" pad="EXP@10"/>
<connect gate="EXP" pin="EXP@11" pad="EXP@11"/>
<connect gate="EXP" pin="EXP@12" pad="EXP@12"/>
<connect gate="EXP" pin="EXP@13" pad="EXP@13"/>
<connect gate="EXP" pin="EXP@14" pad="EXP@14"/>
<connect gate="EXP" pin="EXP@15" pad="EXP@15"/>
<connect gate="EXP" pin="EXP@16" pad="EXP@16"/>
<connect gate="EXP" pin="EXP@17" pad="EXP@17"/>
<connect gate="EXP" pin="EXP@18" pad="EXP@18"/>
<connect gate="EXP" pin="EXP@2" pad="EXP@2"/>
<connect gate="EXP" pin="EXP@3" pad="EXP@3"/>
<connect gate="EXP" pin="EXP@4" pad="EXP@4"/>
<connect gate="EXP" pin="EXP@5" pad="EXP@5"/>
<connect gate="EXP" pin="EXP@6" pad="EXP@6"/>
<connect gate="EXP" pin="EXP@7" pad="EXP@7"/>
<connect gate="EXP" pin="EXP@8" pad="EXP@8"/>
<connect gate="EXP" pin="EXP@9" pad="EXP@9"/>
<connect gate="G$1" pin="!SD" pad="2"/>
<connect gate="G$1" pin="AGND@1" pad="8"/>
<connect gate="G$1" pin="AGND@2" pad="9"/>
<connect gate="G$1" pin="AVCC@1" pad="19"/>
<connect gate="G$1" pin="AVCC@2" pad="20"/>
<connect gate="G$1" pin="BSL" pad="21"/>
<connect gate="G$1" pin="BSR" pad="16"/>
<connect gate="G$1" pin="BYPASS" pad="7"/>
<connect gate="G$1" pin="GAIN0" pad="18"/>
<connect gate="G$1" pin="GAIN1" pad="17"/>
<connect gate="G$1" pin="LIN" pad="5"/>
<connect gate="G$1" pin="LOUT" pad="22"/>
<connect gate="G$1" pin="MUTE" pad="4"/>
<connect gate="G$1" pin="PGNDL@1" pad="23"/>
<connect gate="G$1" pin="PGNDL@2" pad="24"/>
<connect gate="G$1" pin="PGNDR@1" pad="13"/>
<connect gate="G$1" pin="PGNDR@2" pad="14"/>
<connect gate="G$1" pin="PVCCL@1" pad="1"/>
<connect gate="G$1" pin="PVCCL@2" pad="3"/>
<connect gate="G$1" pin="PVCCR@1" pad="10"/>
<connect gate="G$1" pin="PVCCR@2" pad="12"/>
<connect gate="G$1" pin="RIN" pad="6"/>
<connect gate="G$1" pin="ROUT" pad="15"/>
<connect gate="G$1" pin="VCLAMP" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPA3123D2PWP"/>
<attribute name="OC_FARNELL" value="1632099"/>
<attribute name="OC_NEWARK" value="53M3994"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430FG437" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/msp430fg437.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430FG437"/>
</gates>
<devices>
<device name="" package="PN_S-PQFP-G80">
<connects>
<connect gate="G$1" pin="AVCC" pad="80"/>
<connect gate="G$1" pin="AVSS" pad="78"/>
<connect gate="G$1" pin="COM0" pad="44"/>
<connect gate="G$1" pin="DVCC1" pad="1"/>
<connect gate="G$1" pin="DVCC2" pad="52"/>
<connect gate="G$1" pin="DVSS1" pad="79"/>
<connect gate="G$1" pin="DVSS2" pad="53"/>
<connect gate="G$1" pin="P1_0/TA0" pad="67"/>
<connect gate="G$1" pin="P1_1/TA0/MCLK" pad="66"/>
<connect gate="G$1" pin="P1_2/TA1" pad="65"/>
<connect gate="G$1" pin="P1_3/TBOUTH/SVSOUT" pad="64"/>
<connect gate="G$1" pin="P1_4/TBCLK/SMCLK" pad="63"/>
<connect gate="G$1" pin="P1_5/TACLK/ACLK" pad="62"/>
<connect gate="G$1" pin="P1_6/CA0" pad="61"/>
<connect gate="G$1" pin="P1_7/CA13" pad="60"/>
<connect gate="G$1" pin="P2_0/TA2" pad="59"/>
<connect gate="G$1" pin="P2_1/TB0" pad="58"/>
<connect gate="G$1" pin="P2_2/TB1" pad="57"/>
<connect gate="G$1" pin="P2_3/TB2" pad="56"/>
<connect gate="G$1" pin="P2_4/UTXD0" pad="55"/>
<connect gate="G$1" pin="P2_5/URXD0" pad="54"/>
<connect gate="G$1" pin="P2_6/CAOUT/S19" pad="31"/>
<connect gate="G$1" pin="P2_7/ADC12CLK/S18" pad="30"/>
<connect gate="G$1" pin="P3_0/STE0/S31" pad="43"/>
<connect gate="G$1" pin="P3_1/SIMO0/S30" pad="42"/>
<connect gate="G$1" pin="P3_2/SOMI0/S29" pad="41"/>
<connect gate="G$1" pin="P3_3/UCLK0/S28" pad="40"/>
<connect gate="G$1" pin="P3_4/S27" pad="39"/>
<connect gate="G$1" pin="P3_5/S26" pad="38"/>
<connect gate="G$1" pin="P3_6/S25/DMAE0" pad="37"/>
<connect gate="G$1" pin="P3_7/S24" pad="36"/>
<connect gate="G$1" pin="P4_0/S9" pad="21"/>
<connect gate="G$1" pin="P4_1/S8" pad="20"/>
<connect gate="G$1" pin="P4_2/S7" pad="19"/>
<connect gate="G$1" pin="P4_3/S6" pad="18"/>
<connect gate="G$1" pin="P4_4/S5" pad="17"/>
<connect gate="G$1" pin="P4_5/S4" pad="16"/>
<connect gate="G$1" pin="P4_6/S3/A15" pad="15"/>
<connect gate="G$1" pin="P4_7/S2/A14" pad="14"/>
<connect gate="G$1" pin="P5_0/S1/A13" pad="13"/>
<connect gate="G$1" pin="P5_1/S0/A12/DAC1" pad="12"/>
<connect gate="G$1" pin="P5_2/COM1" pad="45"/>
<connect gate="G$1" pin="P5_3/COM2" pad="46"/>
<connect gate="G$1" pin="P5_4/COM3" pad="47"/>
<connect gate="G$1" pin="P5_5/R13" pad="49"/>
<connect gate="G$1" pin="P5_6/R23" pad="50"/>
<connect gate="G$1" pin="P5_7/R33" pad="51"/>
<connect gate="G$1" pin="P6_0/A0/OA0I0" pad="75"/>
<connect gate="G$1" pin="P6_1/A1/OA0O" pad="76"/>
<connect gate="G$1" pin="P6_2/A2/OA0I1" pad="77"/>
<connect gate="G$1" pin="P6_3/A3/OA1I1/OA1O" pad="2"/>
<connect gate="G$1" pin="P6_4/A4/OA1I0" pad="3"/>
<connect gate="G$1" pin="P6_5/A5/OA2I1/OA2O" pad="4"/>
<connect gate="G$1" pin="P6_6/A6/DAC0/OA2I0" pad="5"/>
<connect gate="G$1" pin="P6_7/A7/DAC1/SVSIN" pad="6"/>
<connect gate="G$1" pin="R03" pad="48"/>
<connect gate="G$1" pin="RST/NMI" pad="74"/>
<connect gate="G$1" pin="S10" pad="22"/>
<connect gate="G$1" pin="S11" pad="23"/>
<connect gate="G$1" pin="S12" pad="24"/>
<connect gate="G$1" pin="S13" pad="25"/>
<connect gate="G$1" pin="S14" pad="26"/>
<connect gate="G$1" pin="S15" pad="27"/>
<connect gate="G$1" pin="S16" pad="28"/>
<connect gate="G$1" pin="S17" pad="29"/>
<connect gate="G$1" pin="S20" pad="32"/>
<connect gate="G$1" pin="S21" pad="33"/>
<connect gate="G$1" pin="S22" pad="34"/>
<connect gate="G$1" pin="S23" pad="35"/>
<connect gate="G$1" pin="TCK" pad="73"/>
<connect gate="G$1" pin="TDI/TCLK" pad="71"/>
<connect gate="G$1" pin="TDO/TDI" pad="70"/>
<connect gate="G$1" pin="TMS" pad="72"/>
<connect gate="G$1" pin="VEREF+/DAC0" pad="10"/>
<connect gate="G$1" pin="VREF+" pad="7"/>
<connect gate="G$1" pin="VREF-/VEREF-" pad="11"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT" pad="9"/>
<connect gate="G$1" pin="XT2IN" pad="69"/>
<connect gate="G$1" pin="XT2OUT" pad="68"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430FG437IPN"/>
<attribute name="OC_FARNELL" value="1471275"/>
<attribute name="OC_NEWARK" value="61M7844"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6108*" prefix="IC">
<description>&lt;b&gt;HIGH VOLTAGE DC/DC BOOST CONVERTER WITH 0.5-A/1.3-A INTEGRATED SWITCH&lt;/b&gt;&lt;p&gt;
Source: www.ti.com .. tps61081[1].pdf</description>
<gates>
<gate name="G$1" symbol="TPS6108"/>
<gate name="EXP" symbol="EXP-3"/>
</gates>
<devices>
<device name="" package="S-PDSO-N10">
<connects>
<connect gate="EXP" pin="EXP@1" pad="PP"/>
<connect gate="EXP" pin="EXP@2" pad="PP@1"/>
<connect gate="EXP" pin="EXP@3" pad="PP@2"/>
<connect gate="G$1" pin="EN" pad="6"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="FSW" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="L" pad="1"/>
<connect gate="G$1" pin="OUT" pad="9"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="SS" pad="3"/>
<connect gate="G$1" pin="SW" pad="10"/>
<connect gate="G$1" pin="VIN" pad="2"/>
</connects>
<technologies>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS61080DRCT"/>
<attribute name="OC_FARNELL" value="1412517"/>
<attribute name="OC_NEWARK" value="30M1831"/>
</technology>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS61081DRCT"/>
<attribute name="OC_FARNELL" value="1412518"/>
<attribute name="OC_NEWARK" value="30M1833"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRC4392" prefix="IC">
<description>&lt;b&gt;Two-Channel, Asynchronous Sample Rate Converter with Integrated Digital Audio Interface Receiver and Transmitter&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/src4392.pdf</description>
<gates>
<gate name="G$1" symbol="SRC4392"/>
</gates>
<devices>
<device name="" package="S-PQFP-G48">
<connects>
<connect gate="G$1" pin="!CS!/A0" pad="19"/>
<connect gate="G$1" pin="!INT" pad="23"/>
<connect gate="G$1" pin="!LOCK" pad="11"/>
<connect gate="G$1" pin="!RDY" pad="15"/>
<connect gate="G$1" pin="!RST" pad="24"/>
<connect gate="G$1" pin="AESOUT" pad="34"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCKA" pad="37"/>
<connect gate="G$1" pin="BCKB" pad="48"/>
<connect gate="G$1" pin="BGND" pad="44"/>
<connect gate="G$1" pin="BLS" pad="35"/>
<connect gate="G$1" pin="CCLK/SCL" pad="20"/>
<connect gate="G$1" pin="CDIN/A1" pad="21"/>
<connect gate="G$1" pin="CDOUT/SDA" pad="22"/>
<connect gate="G$1" pin="CPM" pad="18"/>
<connect gate="G$1" pin="DGND1" pad="16"/>
<connect gate="G$1" pin="DGND2" pad="30"/>
<connect gate="G$1" pin="DGND3" pad="43"/>
<connect gate="G$1" pin="GPO1" pad="26"/>
<connect gate="G$1" pin="GPO2" pad="27"/>
<connect gate="G$1" pin="GPO3" pad="28"/>
<connect gate="G$1" pin="GPO4" pad="29"/>
<connect gate="G$1" pin="LRCKA" pad="38"/>
<connect gate="G$1" pin="LRCKB" pad="47"/>
<connect gate="G$1" pin="MCLK" pad="25"/>
<connect gate="G$1" pin="MUTE" pad="14"/>
<connect gate="G$1" pin="RX1+" pad="1"/>
<connect gate="G$1" pin="RX1-" pad="2"/>
<connect gate="G$1" pin="RX2+" pad="3"/>
<connect gate="G$1" pin="RX2-" pad="4"/>
<connect gate="G$1" pin="RX3+" pad="5"/>
<connect gate="G$1" pin="RX3-" pad="6"/>
<connect gate="G$1" pin="RX4+" pad="7"/>
<connect gate="G$1" pin="RX4-" pad="8"/>
<connect gate="G$1" pin="RXCKI" pad="13"/>
<connect gate="G$1" pin="RXCKO" pad="12"/>
<connect gate="G$1" pin="SDINA" pad="39"/>
<connect gate="G$1" pin="SDINB" pad="46"/>
<connect gate="G$1" pin="SDOUTA" pad="40"/>
<connect gate="G$1" pin="SDOUTB" pad="45"/>
<connect gate="G$1" pin="SYNC" pad="36"/>
<connect gate="G$1" pin="TX+" pad="32"/>
<connect gate="G$1" pin="TX-" pad="31"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VDD18" pad="17"/>
<connect gate="G$1" pin="VDD33" pad="33"/>
<connect gate="G$1" pin="VIO" pad="42"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SRC4392IPFB"/>
<attribute name="OC_FARNELL" value="1624400"/>
<attribute name="OC_NEWARK" value="01P4068"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRC4382" prefix="IC">
<description>&lt;b&gt;Two-Channel, Asynchronous Sample Rate Converter with Integrated Digital Audio Interface Receiver and Transmitter&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/src4382.pdf</description>
<gates>
<gate name="G$1" symbol="SRC4382"/>
</gates>
<devices>
<device name="" package="S-PQFP-G48">
<connects>
<connect gate="G$1" pin="!CS!/A0" pad="19"/>
<connect gate="G$1" pin="!INT" pad="23"/>
<connect gate="G$1" pin="!LOCK" pad="11"/>
<connect gate="G$1" pin="!RDY" pad="15"/>
<connect gate="G$1" pin="!RST" pad="24"/>
<connect gate="G$1" pin="AESOUT" pad="34"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCKA" pad="37"/>
<connect gate="G$1" pin="BCKB" pad="48"/>
<connect gate="G$1" pin="BGND" pad="44"/>
<connect gate="G$1" pin="BLS" pad="35"/>
<connect gate="G$1" pin="CCLK/SCL" pad="20"/>
<connect gate="G$1" pin="CDIN/A1" pad="21"/>
<connect gate="G$1" pin="CDOUT/SDA" pad="22"/>
<connect gate="G$1" pin="CPM" pad="18"/>
<connect gate="G$1" pin="DGND1" pad="16"/>
<connect gate="G$1" pin="DGND2" pad="30"/>
<connect gate="G$1" pin="DGND3" pad="43"/>
<connect gate="G$1" pin="GPO1" pad="26"/>
<connect gate="G$1" pin="GPO2" pad="27"/>
<connect gate="G$1" pin="GPO3" pad="28"/>
<connect gate="G$1" pin="GPO4" pad="29"/>
<connect gate="G$1" pin="LRCKA" pad="38"/>
<connect gate="G$1" pin="LRCKB" pad="47"/>
<connect gate="G$1" pin="MCLK" pad="25"/>
<connect gate="G$1" pin="MUTE" pad="14"/>
<connect gate="G$1" pin="NC" pad="41"/>
<connect gate="G$1" pin="RX1+" pad="1"/>
<connect gate="G$1" pin="RX1-" pad="2"/>
<connect gate="G$1" pin="RX2+" pad="3"/>
<connect gate="G$1" pin="RX2-" pad="4"/>
<connect gate="G$1" pin="RX3+" pad="5"/>
<connect gate="G$1" pin="RX3-" pad="6"/>
<connect gate="G$1" pin="RX4+" pad="7"/>
<connect gate="G$1" pin="RX4-" pad="8"/>
<connect gate="G$1" pin="RXCKI" pad="13"/>
<connect gate="G$1" pin="RXCKO" pad="12"/>
<connect gate="G$1" pin="SDINA" pad="39"/>
<connect gate="G$1" pin="SDINB" pad="46"/>
<connect gate="G$1" pin="SDOUTA" pad="40"/>
<connect gate="G$1" pin="SDOUTB" pad="45"/>
<connect gate="G$1" pin="SYNC" pad="36"/>
<connect gate="G$1" pin="TX+" pad="32"/>
<connect gate="G$1" pin="TX-" pad="31"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VDD18" pad="17"/>
<connect gate="G$1" pin="VDD33" pad="33"/>
<connect gate="G$1" pin="VIO" pad="42"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SRC4382IPFB"/>
<attribute name="OC_FARNELL" value="1755339"/>
<attribute name="OC_NEWARK" value="99K4322"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIT4192-H" prefix="IC">
<description>&lt;b&gt;192kHz Digital Audio Transmitter&lt;/b&gt; Hardware Mode&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/dit4192.pdf</description>
<gates>
<gate name="G$1" symbol="DIT4192-HARDWARE-MODE"/>
</gates>
<devices>
<device name="" package="PW_R-PDSO-G28">
<connects>
<connect gate="G$1" pin="!AUDIO" pad="22"/>
<connect gate="G$1" pin="!EMPH" pad="23"/>
<connect gate="G$1" pin="!RST" pad="15"/>
<connect gate="G$1" pin="BLS" pad="25"/>
<connect gate="G$1" pin="BLSM" pad="24"/>
<connect gate="G$1" pin="CLK0" pad="5"/>
<connect gate="G$1" pin="CLK1" pad="4"/>
<connect gate="G$1" pin="COPY/C" pad="2"/>
<connect gate="G$1" pin="CSS" pad="1"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="DGND@1" pad="16"/>
<connect gate="G$1" pin="FMT0" pad="9"/>
<connect gate="G$1" pin="FMT1" pad="10"/>
<connect gate="G$1" pin="L" pad="3"/>
<connect gate="G$1" pin="M/!S" pad="14"/>
<connect gate="G$1" pin="MCLK" pad="6"/>
<connect gate="G$1" pin="MDAT" pad="20"/>
<connect gate="G$1" pin="MODE" pad="28"/>
<connect gate="G$1" pin="MONO" pad="21"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDATA" pad="13"/>
<connect gate="G$1" pin="SYNC" pad="12"/>
<connect gate="G$1" pin="TX+" pad="18"/>
<connect gate="G$1" pin="TX-" pad="17"/>
<connect gate="G$1" pin="U" pad="27"/>
<connect gate="G$1" pin="V" pad="26"/>
<connect gate="G$1" pin="VDD" pad="19"/>
<connect gate="G$1" pin="VIO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DIT4192IPW"/>
<attribute name="OC_FARNELL" value="7455057"/>
<attribute name="OC_NEWARK" value="74C9511"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIT4192-S" prefix="IC">
<description>&lt;b&gt;192kHz Digital Audio Transmitter&lt;/b&gt; Software Mode&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/dit4192.pdf</description>
<gates>
<gate name="G$1" symbol="DIT4192-SOFTWARE-MODE"/>
</gates>
<devices>
<device name="" package="PW_R-PDSO-G28">
<connects>
<connect gate="G$1" pin="!CS" pad="5"/>
<connect gate="G$1" pin="!INT" pad="22"/>
<connect gate="G$1" pin="!RST" pad="15"/>
<connect gate="G$1" pin="BLS" pad="25"/>
<connect gate="G$1" pin="CCLK" pad="3"/>
<connect gate="G$1" pin="CDIN" pad="4"/>
<connect gate="G$1" pin="CDOUT" pad="2"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="DGND@1" pad="16"/>
<connect gate="G$1" pin="MCLK" pad="6"/>
<connect gate="G$1" pin="MODE" pad="28"/>
<connect gate="G$1" pin="NC" pad="1"/>
<connect gate="G$1" pin="NC@1" pad="10"/>
<connect gate="G$1" pin="NC@2" pad="14"/>
<connect gate="G$1" pin="NC@3" pad="20"/>
<connect gate="G$1" pin="NC@4" pad="21"/>
<connect gate="G$1" pin="NC@5" pad="23"/>
<connect gate="G$1" pin="NC@6" pad="24"/>
<connect gate="G$1" pin="NC@7" pad="26"/>
<connect gate="G$1" pin="RXP" pad="9"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDATA" pad="13"/>
<connect gate="G$1" pin="SYNC" pad="12"/>
<connect gate="G$1" pin="TX+" pad="18"/>
<connect gate="G$1" pin="TX-" pad="17"/>
<connect gate="G$1" pin="U" pad="27"/>
<connect gate="G$1" pin="VDD" pad="19"/>
<connect gate="G$1" pin="VIO" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="DIT4192IPW"/>
<attribute name="OC_FARNELL" value="7455057"/>
<attribute name="OC_NEWARK" value="74C9511"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320C6720*DH" prefix="IC">
<description>&lt;b&gt;Floating-Point Digital Signal Processors&lt;/b&gt;&lt;p&gt;
TMS320C6727B, TMS320C6726B, TMS320C6722B, TMS320C6720&lt;br&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tms320c6720.pdf&lt;br&gt;</description>
<gates>
<gate name="A" symbol="TMS320C6720-1"/>
<gate name="AXI" symbol="TMS320C6720-AXI"/>
<gate name="EM" symbol="TMS320C6720-EM"/>
<gate name="UHPI" symbol="TMS320C6720-UHPI"/>
<gate name="CVDD" symbol="TMS320C6720-CVDD"/>
<gate name="DVDD" symbol="TMS320C6720-DVDD"/>
<gate name="VSS" symbol="TMS320C6720-VSS"/>
</gates>
<devices>
<device name="Z" package="ZDH_S-PBGA-N256">
<connects>
<connect gate="A" pin="ACLKR0" pad="A5"/>
<connect gate="A" pin="ACLKR1" pad="E1"/>
<connect gate="A" pin="ACLKR2" pad="C13"/>
<connect gate="A" pin="ACLKX0" pad="A4"/>
<connect gate="A" pin="ACLKX1" pad="E2"/>
<connect gate="A" pin="ACLKX2" pad="D11"/>
<connect gate="A" pin="AFSR0" pad="B4"/>
<connect gate="A" pin="AFSR1" pad="F1"/>
<connect gate="A" pin="AFSR2" pad="C12"/>
<connect gate="A" pin="AFSX0" pad="A3"/>
<connect gate="A" pin="AFSX1" pad="F2"/>
<connect gate="A" pin="AFSX2" pad="C11"/>
<connect gate="A" pin="AHCLKR0/AHCLKR1" pad="B3"/>
<connect gate="A" pin="AHCLKR2" pad="C14"/>
<connect gate="A" pin="AHCLKX0/AHCLKX2" pad="C2"/>
<connect gate="A" pin="AHCLKX1" pad="D1"/>
<connect gate="A" pin="AMUTE0" pad="C1"/>
<connect gate="A" pin="AMUTE1" pad="D2"/>
<connect gate="A" pin="AMUTE2/HINT" pad="D10"/>
<connect gate="A" pin="CLKIN" pad="H2"/>
<connect gate="A" pin="EMU0" pad="M1"/>
<connect gate="A" pin="EMU1" pad="N1"/>
<connect gate="A" pin="OSCIN" pad="J2"/>
<connect gate="A" pin="OSCOUT" pad="J3"/>
<connect gate="A" pin="OSCVDD" pad="J4"/>
<connect gate="A" pin="OSCVSS" pad="J1"/>
<connect gate="A" pin="PLLHV" pad="K2"/>
<connect gate="A" pin="RESET" pad="G2"/>
<connect gate="A" pin="SPI0_CLK/I2C0_SCL" pad="C16"/>
<connect gate="A" pin="SPI0_ENA/I2C1_SDA" pad="D16"/>
<connect gate="A" pin="SPI0_SCS/I2C1_SCL" pad="C15"/>
<connect gate="A" pin="SPI0_SIMO" pad="B15"/>
<connect gate="A" pin="SPI0_SOMI/I2C0_SDA" pad="B14"/>
<connect gate="A" pin="TCK" pad="P1"/>
<connect gate="A" pin="TDI" pad="L1"/>
<connect gate="A" pin="TDO" pad="M2"/>
<connect gate="A" pin="TMS" pad="K3"/>
<connect gate="A" pin="TRST" pad="K4"/>
<connect gate="AXI" pin="AXR00" pad="A14"/>
<connect gate="AXI" pin="AXR01" pad="B13"/>
<connect gate="AXI" pin="AXR010/AXR13" pad="B8"/>
<connect gate="AXI" pin="AXR011/AXR12" pad="A8"/>
<connect gate="AXI" pin="AXR012/AXR11" pad="B7"/>
<connect gate="AXI" pin="AXR013/AXR10" pad="B6"/>
<connect gate="AXI" pin="AXR014/AXR21" pad="A6"/>
<connect gate="AXI" pin="AXR015/AXR20" pad="B5"/>
<connect gate="AXI" pin="AXR02" pad="A13"/>
<connect gate="AXI" pin="AXR03" pad="B12"/>
<connect gate="AXI" pin="AXR04" pad="A12"/>
<connect gate="AXI" pin="AXR05/SPI1_SCS" pad="B11"/>
<connect gate="AXI" pin="AXR06/SPI1_ENA" pad="A11"/>
<connect gate="AXI" pin="AXR07/SPI1_CLK" pad="B10"/>
<connect gate="AXI" pin="AXR08/AXR15/SPI1_SOMI" pad="B9"/>
<connect gate="AXI" pin="AXR09/AXR14/SPI1_SIMO" pad="A9"/>
<connect gate="CVDD" pin="CVDD" pad="E6"/>
<connect gate="CVDD" pin="CVDD@1" pad="E7"/>
<connect gate="CVDD" pin="CVDD@10" pad="J5"/>
<connect gate="CVDD" pin="CVDD@11" pad="J12"/>
<connect gate="CVDD" pin="CVDD@12" pad="K5"/>
<connect gate="CVDD" pin="CVDD@13" pad="K12"/>
<connect gate="CVDD" pin="CVDD@14" pad="M6"/>
<connect gate="CVDD" pin="CVDD@15" pad="M7"/>
<connect gate="CVDD" pin="CVDD@16" pad="M8"/>
<connect gate="CVDD" pin="CVDD@17" pad="M9"/>
<connect gate="CVDD" pin="CVDD@18" pad="M10"/>
<connect gate="CVDD" pin="CVDD@19" pad="M11"/>
<connect gate="CVDD" pin="CVDD@2" pad="E8"/>
<connect gate="CVDD" pin="CVDD@3" pad="E9"/>
<connect gate="CVDD" pin="CVDD@4" pad="E10"/>
<connect gate="CVDD" pin="CVDD@5" pad="E11"/>
<connect gate="CVDD" pin="CVDD@6" pad="G5"/>
<connect gate="CVDD" pin="CVDD@7" pad="G12"/>
<connect gate="CVDD" pin="CVDD@8" pad="H5"/>
<connect gate="CVDD" pin="CVDD@9" pad="H12"/>
<connect gate="DVDD" pin="DVDD" pad="A2"/>
<connect gate="DVDD" pin="DVDD@1" pad="A15"/>
<connect gate="DVDD" pin="DVDD@10" pad="J14"/>
<connect gate="DVDD" pin="DVDD@11" pad="M4"/>
<connect gate="DVDD" pin="DVDD@12" pad="M13"/>
<connect gate="DVDD" pin="DVDD@13" pad="N5"/>
<connect gate="DVDD" pin="DVDD@14" pad="N12"/>
<connect gate="DVDD" pin="DVDD@15" pad="P8"/>
<connect gate="DVDD" pin="DVDD@16" pad="R1"/>
<connect gate="DVDD" pin="DVDD@17" pad="R16"/>
<connect gate="DVDD" pin="DVDD@18" pad="T2"/>
<connect gate="DVDD" pin="DVDD@19" pad="T15"/>
<connect gate="DVDD" pin="DVDD@2" pad="B1"/>
<connect gate="DVDD" pin="DVDD@3" pad="B16"/>
<connect gate="DVDD" pin="DVDD@4" pad="D4"/>
<connect gate="DVDD" pin="DVDD@5" pad="D5"/>
<connect gate="DVDD" pin="DVDD@6" pad="D12"/>
<connect gate="DVDD" pin="DVDD@7" pad="D13"/>
<connect gate="DVDD" pin="DVDD@8" pad="E4"/>
<connect gate="DVDD" pin="DVDD@9" pad="E13"/>
<connect gate="EM" pin="EM_A0" pad="J16"/>
<connect gate="EM" pin="EM_A1" pad="J15"/>
<connect gate="EM" pin="EM_A10" pad="H15"/>
<connect gate="EM" pin="EM_A11" pad="P15"/>
<connect gate="EM" pin="EM_A12" pad="P12"/>
<connect gate="EM" pin="EM_A2" pad="K15"/>
<connect gate="EM" pin="EM_A3" pad="L16"/>
<connect gate="EM" pin="EM_A4" pad="L15"/>
<connect gate="EM" pin="EM_A5" pad="M16"/>
<connect gate="EM" pin="EM_A6" pad="M15"/>
<connect gate="EM" pin="EM_A7" pad="N16"/>
<connect gate="EM" pin="EM_A8" pad="N15"/>
<connect gate="EM" pin="EM_A9" pad="P16"/>
<connect gate="EM" pin="EM_BA0" pad="G15"/>
<connect gate="EM" pin="EM_BA1" pad="H16"/>
<connect gate="EM" pin="EM_CAS" pad="R3"/>
<connect gate="EM" pin="EM_CKE" pad="T14"/>
<connect gate="EM" pin="EM_CLK" pad="R14"/>
<connect gate="EM" pin="EM_CS0" pad="F15"/>
<connect gate="EM" pin="EM_CS2" pad="E15"/>
<connect gate="EM" pin="EM_D0" pad="T8"/>
<connect gate="EM" pin="EM_D1" pad="R8"/>
<connect gate="EM" pin="EM_D10" pad="R12"/>
<connect gate="EM" pin="EM_D11" pad="T11"/>
<connect gate="EM" pin="EM_D12" pad="R11"/>
<connect gate="EM" pin="EM_D13" pad="R10"/>
<connect gate="EM" pin="EM_D14" pad="T9"/>
<connect gate="EM" pin="EM_D15" pad="R9"/>
<connect gate="EM" pin="EM_D16/UHPI_HA0" pad="N7"/>
<connect gate="EM" pin="EM_D17/UHPI_HA1" pad="P6"/>
<connect gate="EM" pin="EM_D18/UHPI_HA2" pad="N6"/>
<connect gate="EM" pin="EM_D19/UHPI_HA3" pad="P5"/>
<connect gate="EM" pin="EM_D2" pad="R7"/>
<connect gate="EM" pin="EM_D20/UHPI_HA4" pad="P4"/>
<connect gate="EM" pin="EM_D21/UHPI_HA5" pad="P3"/>
<connect gate="EM" pin="EM_D22/UHPI_HA6" pad="N4"/>
<connect gate="EM" pin="EM_D23/UHPI_HA7" pad="R2"/>
<connect gate="EM" pin="EM_D24/UHPI_HA8" pad="P11"/>
<connect gate="EM" pin="EM_D25/UHPI_HA9" pad="N11"/>
<connect gate="EM" pin="EM_D26/UHPI_HA10" pad="P10"/>
<connect gate="EM" pin="EM_D27/UHPI_HA11" pad="N10"/>
<connect gate="EM" pin="EM_D28/UHPI_HA12" pad="P9"/>
<connect gate="EM" pin="EM_D29/UHPI_HA13" pad="N9"/>
<connect gate="EM" pin="EM_D3" pad="T6"/>
<connect gate="EM" pin="EM_D30/UHPI_HA14" pad="N8"/>
<connect gate="EM" pin="EM_D31/UHPI_HA15" pad="P7"/>
<connect gate="EM" pin="EM_D4" pad="R6"/>
<connect gate="EM" pin="EM_D5" pad="T5"/>
<connect gate="EM" pin="EM_D6" pad="R5"/>
<connect gate="EM" pin="EM_D7" pad="T4"/>
<connect gate="EM" pin="EM_D8" pad="R13"/>
<connect gate="EM" pin="EM_D9" pad="T12"/>
<connect gate="EM" pin="EM_OE" pad="D15"/>
<connect gate="EM" pin="EM_RAS" pad="F16"/>
<connect gate="EM" pin="EM_RW" pad="E16"/>
<connect gate="EM" pin="EM_WAIT" pad="D14"/>
<connect gate="EM" pin="EM_WE" pad="T3"/>
<connect gate="EM" pin="EM_WE_DQM0" pad="R4"/>
<connect gate="EM" pin="EM_WE_DQM1" pad="T13"/>
<connect gate="EM" pin="EM_WE_DQM2" pad="P13"/>
<connect gate="EM" pin="EM_WE_DQM3" pad="R15"/>
<connect gate="UHPI" pin="UHPI_HAS" pad="C9"/>
<connect gate="UHPI" pin="UHPI_HBE0" pad="C6"/>
<connect gate="UHPI" pin="UHPI_HBE1" pad="C5"/>
<connect gate="UHPI" pin="UHPI_HBE2" pad="C4"/>
<connect gate="UHPI" pin="UHPI_HBE3" pad="B2"/>
<connect gate="UHPI" pin="UHPI_HCNTL0" pad="D9"/>
<connect gate="UHPI" pin="UHPI_HCNTL1" pad="C10"/>
<connect gate="UHPI" pin="UHPI_HCS" pad="C8"/>
<connect gate="UHPI" pin="UHPI_HD0" pad="K13"/>
<connect gate="UHPI" pin="UHPI_HD1" pad="K14"/>
<connect gate="UHPI" pin="UHPI_HD10" pad="F13"/>
<connect gate="UHPI" pin="UHPI_HD11" pad="G14"/>
<connect gate="UHPI" pin="UHPI_HD12" pad="G13"/>
<connect gate="UHPI" pin="UHPI_HD13" pad="H14"/>
<connect gate="UHPI" pin="UHPI_HD14" pad="H13"/>
<connect gate="UHPI" pin="UHPI_HD15" pad="J13"/>
<connect gate="UHPI" pin="UHPI_HD16/HHWIL" pad="H1"/>
<connect gate="UHPI" pin="UHPI_HD17" pad="G3"/>
<connect gate="UHPI" pin="UHPI_HD18" pad="G4"/>
<connect gate="UHPI" pin="UHPI_HD19" pad="F3"/>
<connect gate="UHPI" pin="UHPI_HD2" pad="M14"/>
<connect gate="UHPI" pin="UHPI_HD20" pad="F4"/>
<connect gate="UHPI" pin="UHPI_HD21" pad="E3"/>
<connect gate="UHPI" pin="UHPI_HD22" pad="D3"/>
<connect gate="UHPI" pin="UHPI_HD23" pad="C3"/>
<connect gate="UHPI" pin="UHPI_HD24" pad="P2"/>
<connect gate="UHPI" pin="UHPI_HD25" pad="N2"/>
<connect gate="UHPI" pin="UHPI_HD26" pad="N3"/>
<connect gate="UHPI" pin="UHPI_HD27" pad="M3"/>
<connect gate="UHPI" pin="UHPI_HD28" pad="L3"/>
<connect gate="UHPI" pin="UHPI_HD29" pad="L4"/>
<connect gate="UHPI" pin="UHPI_HD3" pad="L13"/>
<connect gate="UHPI" pin="UHPI_HD30" pad="L2"/>
<connect gate="UHPI" pin="UHPI_HD31" pad="H4"/>
<connect gate="UHPI" pin="UHPI_HD4" pad="L14"/>
<connect gate="UHPI" pin="UHPI_HD5" pad="N13"/>
<connect gate="UHPI" pin="UHPI_HD6" pad="N14"/>
<connect gate="UHPI" pin="UHPI_HD7" pad="P14"/>
<connect gate="UHPI" pin="UHPI_HD8" pad="E14"/>
<connect gate="UHPI" pin="UHPI_HD9" pad="F14"/>
<connect gate="UHPI" pin="UHPI_HDS1" pad="D7"/>
<connect gate="UHPI" pin="UHPI_HDS2" pad="C7"/>
<connect gate="UHPI" pin="UHPI_HRDY" pad="D6"/>
<connect gate="UHPI" pin="UHPI_HRW" pad="D8"/>
<connect gate="VSS" pin="VSS" pad="A1"/>
<connect gate="VSS" pin="VSS@1" pad="A7"/>
<connect gate="VSS" pin="VSS@10" pad="F9"/>
<connect gate="VSS" pin="VSS@11" pad="F10"/>
<connect gate="VSS" pin="VSS@12" pad="F11"/>
<connect gate="VSS" pin="VSS@13" pad="F12"/>
<connect gate="VSS" pin="VSS@14" pad="G1"/>
<connect gate="VSS" pin="VSS@15" pad="G6"/>
<connect gate="VSS" pin="VSS@16" pad="G7"/>
<connect gate="VSS" pin="VSS@17" pad="G8"/>
<connect gate="VSS" pin="VSS@18" pad="G9"/>
<connect gate="VSS" pin="VSS@19" pad="G10"/>
<connect gate="VSS" pin="VSS@2" pad="A10"/>
<connect gate="VSS" pin="VSS@20" pad="G11"/>
<connect gate="VSS" pin="VSS@21" pad="G16"/>
<connect gate="VSS" pin="VSS@22" pad="H3"/>
<connect gate="VSS" pin="VSS@23" pad="H6"/>
<connect gate="VSS" pin="VSS@24" pad="H7"/>
<connect gate="VSS" pin="VSS@25" pad="H8"/>
<connect gate="VSS" pin="VSS@26" pad="H9"/>
<connect gate="VSS" pin="VSS@27" pad="H10"/>
<connect gate="VSS" pin="VSS@28" pad="H11"/>
<connect gate="VSS" pin="VSS@29" pad="J6"/>
<connect gate="VSS" pin="VSS@3" pad="A16"/>
<connect gate="VSS" pin="VSS@30" pad="J7"/>
<connect gate="VSS" pin="VSS@31" pad="J8"/>
<connect gate="VSS" pin="VSS@32" pad="J9"/>
<connect gate="VSS" pin="VSS@33" pad="J10"/>
<connect gate="VSS" pin="VSS@34" pad="J11"/>
<connect gate="VSS" pin="VSS@35" pad="K1"/>
<connect gate="VSS" pin="VSS@36" pad="K6"/>
<connect gate="VSS" pin="VSS@37" pad="K7"/>
<connect gate="VSS" pin="VSS@38" pad="K8"/>
<connect gate="VSS" pin="VSS@39" pad="K9"/>
<connect gate="VSS" pin="VSS@4" pad="E5"/>
<connect gate="VSS" pin="VSS@40" pad="K10"/>
<connect gate="VSS" pin="VSS@41" pad="K11"/>
<connect gate="VSS" pin="VSS@42" pad="K16"/>
<connect gate="VSS" pin="VSS@43" pad="L5"/>
<connect gate="VSS" pin="VSS@44" pad="L6"/>
<connect gate="VSS" pin="VSS@45" pad="L7"/>
<connect gate="VSS" pin="VSS@46" pad="L8"/>
<connect gate="VSS" pin="VSS@47" pad="L9"/>
<connect gate="VSS" pin="VSS@48" pad="L10"/>
<connect gate="VSS" pin="VSS@49" pad="L11"/>
<connect gate="VSS" pin="VSS@5" pad="E12"/>
<connect gate="VSS" pin="VSS@50" pad="L12"/>
<connect gate="VSS" pin="VSS@51" pad="M5"/>
<connect gate="VSS" pin="VSS@52" pad="M12"/>
<connect gate="VSS" pin="VSS@53" pad="T1"/>
<connect gate="VSS" pin="VSS@54" pad="T7"/>
<connect gate="VSS" pin="VSS@55" pad="T10"/>
<connect gate="VSS" pin="VSS@56" pad="T16"/>
<connect gate="VSS" pin="VSS@6" pad="F5"/>
<connect gate="VSS" pin="VSS@7" pad="F6"/>
<connect gate="VSS" pin="VSS@8" pad="F7"/>
<connect gate="VSS" pin="VSS@9" pad="F8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="G" package="GDH_S-PBGA-N256">
<connects>
<connect gate="A" pin="ACLKR0" pad="A5"/>
<connect gate="A" pin="ACLKR1" pad="E1"/>
<connect gate="A" pin="ACLKR2" pad="C13"/>
<connect gate="A" pin="ACLKX0" pad="A4"/>
<connect gate="A" pin="ACLKX1" pad="E2"/>
<connect gate="A" pin="ACLKX2" pad="D11"/>
<connect gate="A" pin="AFSR0" pad="B4"/>
<connect gate="A" pin="AFSR1" pad="F1"/>
<connect gate="A" pin="AFSR2" pad="C12"/>
<connect gate="A" pin="AFSX0" pad="A3"/>
<connect gate="A" pin="AFSX1" pad="F2"/>
<connect gate="A" pin="AFSX2" pad="C11"/>
<connect gate="A" pin="AHCLKR0/AHCLKR1" pad="B3"/>
<connect gate="A" pin="AHCLKR2" pad="C14"/>
<connect gate="A" pin="AHCLKX0/AHCLKX2" pad="C2"/>
<connect gate="A" pin="AHCLKX1" pad="D1"/>
<connect gate="A" pin="AMUTE0" pad="C1"/>
<connect gate="A" pin="AMUTE1" pad="D2"/>
<connect gate="A" pin="AMUTE2/HINT" pad="D10"/>
<connect gate="A" pin="CLKIN" pad="H2"/>
<connect gate="A" pin="EMU0" pad="M1"/>
<connect gate="A" pin="EMU1" pad="N1"/>
<connect gate="A" pin="OSCIN" pad="J2"/>
<connect gate="A" pin="OSCOUT" pad="J3"/>
<connect gate="A" pin="OSCVDD" pad="J4"/>
<connect gate="A" pin="OSCVSS" pad="J1"/>
<connect gate="A" pin="PLLHV" pad="K2"/>
<connect gate="A" pin="RESET" pad="G2"/>
<connect gate="A" pin="SPI0_CLK/I2C0_SCL" pad="C16"/>
<connect gate="A" pin="SPI0_ENA/I2C1_SDA" pad="D16"/>
<connect gate="A" pin="SPI0_SCS/I2C1_SCL" pad="C15"/>
<connect gate="A" pin="SPI0_SIMO" pad="B15"/>
<connect gate="A" pin="SPI0_SOMI/I2C0_SDA" pad="B14"/>
<connect gate="A" pin="TCK" pad="P1"/>
<connect gate="A" pin="TDI" pad="L1"/>
<connect gate="A" pin="TDO" pad="M2"/>
<connect gate="A" pin="TMS" pad="K3"/>
<connect gate="A" pin="TRST" pad="K4"/>
<connect gate="AXI" pin="AXR00" pad="A14"/>
<connect gate="AXI" pin="AXR01" pad="B13"/>
<connect gate="AXI" pin="AXR010/AXR13" pad="B8"/>
<connect gate="AXI" pin="AXR011/AXR12" pad="A8"/>
<connect gate="AXI" pin="AXR012/AXR11" pad="B7"/>
<connect gate="AXI" pin="AXR013/AXR10" pad="B6"/>
<connect gate="AXI" pin="AXR014/AXR21" pad="A6"/>
<connect gate="AXI" pin="AXR015/AXR20" pad="B5"/>
<connect gate="AXI" pin="AXR02" pad="A13"/>
<connect gate="AXI" pin="AXR03" pad="B12"/>
<connect gate="AXI" pin="AXR04" pad="A12"/>
<connect gate="AXI" pin="AXR05/SPI1_SCS" pad="B11"/>
<connect gate="AXI" pin="AXR06/SPI1_ENA" pad="A11"/>
<connect gate="AXI" pin="AXR07/SPI1_CLK" pad="B10"/>
<connect gate="AXI" pin="AXR08/AXR15/SPI1_SOMI" pad="B9"/>
<connect gate="AXI" pin="AXR09/AXR14/SPI1_SIMO" pad="A9"/>
<connect gate="CVDD" pin="CVDD" pad="E6"/>
<connect gate="CVDD" pin="CVDD@1" pad="E7"/>
<connect gate="CVDD" pin="CVDD@10" pad="J5"/>
<connect gate="CVDD" pin="CVDD@11" pad="J12"/>
<connect gate="CVDD" pin="CVDD@12" pad="K5"/>
<connect gate="CVDD" pin="CVDD@13" pad="K12"/>
<connect gate="CVDD" pin="CVDD@14" pad="M6"/>
<connect gate="CVDD" pin="CVDD@15" pad="M7"/>
<connect gate="CVDD" pin="CVDD@16" pad="M8"/>
<connect gate="CVDD" pin="CVDD@17" pad="M9"/>
<connect gate="CVDD" pin="CVDD@18" pad="M10"/>
<connect gate="CVDD" pin="CVDD@19" pad="M11"/>
<connect gate="CVDD" pin="CVDD@2" pad="E8"/>
<connect gate="CVDD" pin="CVDD@3" pad="E9"/>
<connect gate="CVDD" pin="CVDD@4" pad="E10"/>
<connect gate="CVDD" pin="CVDD@5" pad="E11"/>
<connect gate="CVDD" pin="CVDD@6" pad="G5"/>
<connect gate="CVDD" pin="CVDD@7" pad="G12"/>
<connect gate="CVDD" pin="CVDD@8" pad="H5"/>
<connect gate="CVDD" pin="CVDD@9" pad="H12"/>
<connect gate="DVDD" pin="DVDD" pad="A2"/>
<connect gate="DVDD" pin="DVDD@1" pad="A15"/>
<connect gate="DVDD" pin="DVDD@10" pad="J14"/>
<connect gate="DVDD" pin="DVDD@11" pad="M4"/>
<connect gate="DVDD" pin="DVDD@12" pad="M13"/>
<connect gate="DVDD" pin="DVDD@13" pad="N5"/>
<connect gate="DVDD" pin="DVDD@14" pad="N12"/>
<connect gate="DVDD" pin="DVDD@15" pad="P8"/>
<connect gate="DVDD" pin="DVDD@16" pad="R1"/>
<connect gate="DVDD" pin="DVDD@17" pad="R16"/>
<connect gate="DVDD" pin="DVDD@18" pad="T2"/>
<connect gate="DVDD" pin="DVDD@19" pad="T15"/>
<connect gate="DVDD" pin="DVDD@2" pad="B1"/>
<connect gate="DVDD" pin="DVDD@3" pad="B16"/>
<connect gate="DVDD" pin="DVDD@4" pad="D4"/>
<connect gate="DVDD" pin="DVDD@5" pad="D5"/>
<connect gate="DVDD" pin="DVDD@6" pad="D12"/>
<connect gate="DVDD" pin="DVDD@7" pad="D13"/>
<connect gate="DVDD" pin="DVDD@8" pad="E4"/>
<connect gate="DVDD" pin="DVDD@9" pad="E13"/>
<connect gate="EM" pin="EM_A0" pad="J16"/>
<connect gate="EM" pin="EM_A1" pad="J15"/>
<connect gate="EM" pin="EM_A10" pad="H15"/>
<connect gate="EM" pin="EM_A11" pad="P15"/>
<connect gate="EM" pin="EM_A12" pad="P12"/>
<connect gate="EM" pin="EM_A2" pad="K15"/>
<connect gate="EM" pin="EM_A3" pad="L16"/>
<connect gate="EM" pin="EM_A4" pad="L15"/>
<connect gate="EM" pin="EM_A5" pad="M16"/>
<connect gate="EM" pin="EM_A6" pad="M15"/>
<connect gate="EM" pin="EM_A7" pad="N16"/>
<connect gate="EM" pin="EM_A8" pad="N15"/>
<connect gate="EM" pin="EM_A9" pad="P16"/>
<connect gate="EM" pin="EM_BA0" pad="G15"/>
<connect gate="EM" pin="EM_BA1" pad="H16"/>
<connect gate="EM" pin="EM_CAS" pad="R3"/>
<connect gate="EM" pin="EM_CKE" pad="T14"/>
<connect gate="EM" pin="EM_CLK" pad="R14"/>
<connect gate="EM" pin="EM_CS0" pad="F15"/>
<connect gate="EM" pin="EM_CS2" pad="E15"/>
<connect gate="EM" pin="EM_D0" pad="T8"/>
<connect gate="EM" pin="EM_D1" pad="R8"/>
<connect gate="EM" pin="EM_D10" pad="R12"/>
<connect gate="EM" pin="EM_D11" pad="T11"/>
<connect gate="EM" pin="EM_D12" pad="R11"/>
<connect gate="EM" pin="EM_D13" pad="R10"/>
<connect gate="EM" pin="EM_D14" pad="T9"/>
<connect gate="EM" pin="EM_D15" pad="R9"/>
<connect gate="EM" pin="EM_D16/UHPI_HA0" pad="N7"/>
<connect gate="EM" pin="EM_D17/UHPI_HA1" pad="P6"/>
<connect gate="EM" pin="EM_D18/UHPI_HA2" pad="N6"/>
<connect gate="EM" pin="EM_D19/UHPI_HA3" pad="P5"/>
<connect gate="EM" pin="EM_D2" pad="R7"/>
<connect gate="EM" pin="EM_D20/UHPI_HA4" pad="P4"/>
<connect gate="EM" pin="EM_D21/UHPI_HA5" pad="P3"/>
<connect gate="EM" pin="EM_D22/UHPI_HA6" pad="N4"/>
<connect gate="EM" pin="EM_D23/UHPI_HA7" pad="R2"/>
<connect gate="EM" pin="EM_D24/UHPI_HA8" pad="P11"/>
<connect gate="EM" pin="EM_D25/UHPI_HA9" pad="N11"/>
<connect gate="EM" pin="EM_D26/UHPI_HA10" pad="P10"/>
<connect gate="EM" pin="EM_D27/UHPI_HA11" pad="N10"/>
<connect gate="EM" pin="EM_D28/UHPI_HA12" pad="P9"/>
<connect gate="EM" pin="EM_D29/UHPI_HA13" pad="N9"/>
<connect gate="EM" pin="EM_D3" pad="T6"/>
<connect gate="EM" pin="EM_D30/UHPI_HA14" pad="N8"/>
<connect gate="EM" pin="EM_D31/UHPI_HA15" pad="P7"/>
<connect gate="EM" pin="EM_D4" pad="R6"/>
<connect gate="EM" pin="EM_D5" pad="T5"/>
<connect gate="EM" pin="EM_D6" pad="R5"/>
<connect gate="EM" pin="EM_D7" pad="T4"/>
<connect gate="EM" pin="EM_D8" pad="R13"/>
<connect gate="EM" pin="EM_D9" pad="T12"/>
<connect gate="EM" pin="EM_OE" pad="D15"/>
<connect gate="EM" pin="EM_RAS" pad="F16"/>
<connect gate="EM" pin="EM_RW" pad="E16"/>
<connect gate="EM" pin="EM_WAIT" pad="D14"/>
<connect gate="EM" pin="EM_WE" pad="T3"/>
<connect gate="EM" pin="EM_WE_DQM0" pad="R4"/>
<connect gate="EM" pin="EM_WE_DQM1" pad="T13"/>
<connect gate="EM" pin="EM_WE_DQM2" pad="P13"/>
<connect gate="EM" pin="EM_WE_DQM3" pad="R15"/>
<connect gate="UHPI" pin="UHPI_HAS" pad="C9"/>
<connect gate="UHPI" pin="UHPI_HBE0" pad="C6"/>
<connect gate="UHPI" pin="UHPI_HBE1" pad="C5"/>
<connect gate="UHPI" pin="UHPI_HBE2" pad="C4"/>
<connect gate="UHPI" pin="UHPI_HBE3" pad="B2"/>
<connect gate="UHPI" pin="UHPI_HCNTL0" pad="D9"/>
<connect gate="UHPI" pin="UHPI_HCNTL1" pad="C10"/>
<connect gate="UHPI" pin="UHPI_HCS" pad="C8"/>
<connect gate="UHPI" pin="UHPI_HD0" pad="K13"/>
<connect gate="UHPI" pin="UHPI_HD1" pad="K14"/>
<connect gate="UHPI" pin="UHPI_HD10" pad="F13"/>
<connect gate="UHPI" pin="UHPI_HD11" pad="G14"/>
<connect gate="UHPI" pin="UHPI_HD12" pad="G13"/>
<connect gate="UHPI" pin="UHPI_HD13" pad="H14"/>
<connect gate="UHPI" pin="UHPI_HD14" pad="H13"/>
<connect gate="UHPI" pin="UHPI_HD15" pad="J13"/>
<connect gate="UHPI" pin="UHPI_HD16/HHWIL" pad="H1"/>
<connect gate="UHPI" pin="UHPI_HD17" pad="G3"/>
<connect gate="UHPI" pin="UHPI_HD18" pad="G4"/>
<connect gate="UHPI" pin="UHPI_HD19" pad="F3"/>
<connect gate="UHPI" pin="UHPI_HD2" pad="M14"/>
<connect gate="UHPI" pin="UHPI_HD20" pad="F4"/>
<connect gate="UHPI" pin="UHPI_HD21" pad="E3"/>
<connect gate="UHPI" pin="UHPI_HD22" pad="D3"/>
<connect gate="UHPI" pin="UHPI_HD23" pad="C3"/>
<connect gate="UHPI" pin="UHPI_HD24" pad="P2"/>
<connect gate="UHPI" pin="UHPI_HD25" pad="N2"/>
<connect gate="UHPI" pin="UHPI_HD26" pad="N3"/>
<connect gate="UHPI" pin="UHPI_HD27" pad="M3"/>
<connect gate="UHPI" pin="UHPI_HD28" pad="L3"/>
<connect gate="UHPI" pin="UHPI_HD29" pad="L4"/>
<connect gate="UHPI" pin="UHPI_HD3" pad="L13"/>
<connect gate="UHPI" pin="UHPI_HD30" pad="L2"/>
<connect gate="UHPI" pin="UHPI_HD31" pad="H4"/>
<connect gate="UHPI" pin="UHPI_HD4" pad="L14"/>
<connect gate="UHPI" pin="UHPI_HD5" pad="N13"/>
<connect gate="UHPI" pin="UHPI_HD6" pad="N14"/>
<connect gate="UHPI" pin="UHPI_HD7" pad="P14"/>
<connect gate="UHPI" pin="UHPI_HD8" pad="E14"/>
<connect gate="UHPI" pin="UHPI_HD9" pad="F14"/>
<connect gate="UHPI" pin="UHPI_HDS1" pad="D7"/>
<connect gate="UHPI" pin="UHPI_HDS2" pad="C7"/>
<connect gate="UHPI" pin="UHPI_HRDY" pad="D6"/>
<connect gate="UHPI" pin="UHPI_HRW" pad="D8"/>
<connect gate="VSS" pin="VSS" pad="A1"/>
<connect gate="VSS" pin="VSS@1" pad="A7"/>
<connect gate="VSS" pin="VSS@10" pad="F9"/>
<connect gate="VSS" pin="VSS@11" pad="F10"/>
<connect gate="VSS" pin="VSS@12" pad="F11"/>
<connect gate="VSS" pin="VSS@13" pad="F12"/>
<connect gate="VSS" pin="VSS@14" pad="G1"/>
<connect gate="VSS" pin="VSS@15" pad="G6"/>
<connect gate="VSS" pin="VSS@16" pad="G7"/>
<connect gate="VSS" pin="VSS@17" pad="G8"/>
<connect gate="VSS" pin="VSS@18" pad="G9"/>
<connect gate="VSS" pin="VSS@19" pad="G10"/>
<connect gate="VSS" pin="VSS@2" pad="A10"/>
<connect gate="VSS" pin="VSS@20" pad="G11"/>
<connect gate="VSS" pin="VSS@21" pad="G16"/>
<connect gate="VSS" pin="VSS@22" pad="H3"/>
<connect gate="VSS" pin="VSS@23" pad="H6"/>
<connect gate="VSS" pin="VSS@24" pad="H7"/>
<connect gate="VSS" pin="VSS@25" pad="H8"/>
<connect gate="VSS" pin="VSS@26" pad="H9"/>
<connect gate="VSS" pin="VSS@27" pad="H10"/>
<connect gate="VSS" pin="VSS@28" pad="H11"/>
<connect gate="VSS" pin="VSS@29" pad="J6"/>
<connect gate="VSS" pin="VSS@3" pad="A16"/>
<connect gate="VSS" pin="VSS@30" pad="J7"/>
<connect gate="VSS" pin="VSS@31" pad="J8"/>
<connect gate="VSS" pin="VSS@32" pad="J9"/>
<connect gate="VSS" pin="VSS@33" pad="J10"/>
<connect gate="VSS" pin="VSS@34" pad="J11"/>
<connect gate="VSS" pin="VSS@35" pad="K1"/>
<connect gate="VSS" pin="VSS@36" pad="K6"/>
<connect gate="VSS" pin="VSS@37" pad="K7"/>
<connect gate="VSS" pin="VSS@38" pad="K8"/>
<connect gate="VSS" pin="VSS@39" pad="K9"/>
<connect gate="VSS" pin="VSS@4" pad="E5"/>
<connect gate="VSS" pin="VSS@40" pad="K10"/>
<connect gate="VSS" pin="VSS@41" pad="K11"/>
<connect gate="VSS" pin="VSS@42" pad="K16"/>
<connect gate="VSS" pin="VSS@43" pad="L5"/>
<connect gate="VSS" pin="VSS@44" pad="L6"/>
<connect gate="VSS" pin="VSS@45" pad="L7"/>
<connect gate="VSS" pin="VSS@46" pad="L8"/>
<connect gate="VSS" pin="VSS@47" pad="L9"/>
<connect gate="VSS" pin="VSS@48" pad="L10"/>
<connect gate="VSS" pin="VSS@49" pad="L11"/>
<connect gate="VSS" pin="VSS@5" pad="E12"/>
<connect gate="VSS" pin="VSS@50" pad="L12"/>
<connect gate="VSS" pin="VSS@51" pad="M5"/>
<connect gate="VSS" pin="VSS@52" pad="M12"/>
<connect gate="VSS" pin="VSS@53" pad="T1"/>
<connect gate="VSS" pin="VSS@54" pad="T7"/>
<connect gate="VSS" pin="VSS@55" pad="T10"/>
<connect gate="VSS" pin="VSS@56" pad="T16"/>
<connect gate="VSS" pin="VSS@6" pad="F5"/>
<connect gate="VSS" pin="VSS@7" pad="F6"/>
<connect gate="VSS" pin="VSS@8" pad="F7"/>
<connect gate="VSS" pin="VSS@9" pad="F8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320C6720RFP-EXPAD" prefix="IC">
<description>&lt;b&gt;Floating-Point Digital Signal Processors&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tms320c6720.pdf&lt;br&gt;</description>
<gates>
<gate name="A" symbol="TMS320C6720-QFP-A"/>
<gate name="EM" symbol="TMS320C6720-QFP-EM"/>
<gate name="CVDD" symbol="TMS320C6720-QFP-CVDD"/>
<gate name="DVDD" symbol="TMS320C6720-QFP-DVDD"/>
<gate name="VSS" symbol="TMS320C6720-QFP-VSS"/>
<gate name="EXP" symbol="EXP-100"/>
</gates>
<devices>
<device name="" package="RFP_S-PQFP-G144-EXPAD">
<connects>
<connect gate="A" pin="ACLKR0" pad="139"/>
<connect gate="A" pin="ACLKR1" pad="9"/>
<connect gate="A" pin="ACLKX0" pad="142"/>
<connect gate="A" pin="ACLKX1" pad="7"/>
<connect gate="A" pin="AFSR0" pad="141"/>
<connect gate="A" pin="AFSR1" pad="12"/>
<connect gate="A" pin="AFSX0" pad="144"/>
<connect gate="A" pin="AFSX1" pad="11"/>
<connect gate="A" pin="AHCLKR0/AHCLKR1" pad="143"/>
<connect gate="A" pin="AHCLKX0/AHCLKX2" pad="2"/>
<connect gate="A" pin="AHCLKX1" pad="5"/>
<connect gate="A" pin="AMUTE0" pad="3"/>
<connect gate="A" pin="AMUTE1" pad="4"/>
<connect gate="A" pin="AXR00" pad="113"/>
<connect gate="A" pin="AXR01" pad="115"/>
<connect gate="A" pin="AXR010/AXR13" pad="130"/>
<connect gate="A" pin="AXR011/AXR12" pad="131"/>
<connect gate="A" pin="AXR012/AXR11" pad="134"/>
<connect gate="A" pin="AXR013/AXR10" pad="135"/>
<connect gate="A" pin="AXR014/AXR21" pad="137"/>
<connect gate="A" pin="AXR015/AXR20" pad="138"/>
<connect gate="A" pin="AXR02" pad="116"/>
<connect gate="A" pin="AXR03" pad="117"/>
<connect gate="A" pin="AXR04" pad="119"/>
<connect gate="A" pin="AXR05/SPI1_SCS" pad="120"/>
<connect gate="A" pin="AXR06/SPI1_ENA" pad="121"/>
<connect gate="A" pin="AXR07/SPI1_CLK" pad="122"/>
<connect gate="A" pin="AXR08/AXR15/SPI1_SOMI" pad="126"/>
<connect gate="A" pin="AXR09/AXR14/SPI1_SIMO" pad="127"/>
<connect gate="A" pin="CLKIN" pad="17"/>
<connect gate="A" pin="EMU0" pad="32"/>
<connect gate="A" pin="EMU1" pad="34"/>
<connect gate="A" pin="OSCIN" pad="23"/>
<connect gate="A" pin="OSCOUT" pad="24"/>
<connect gate="A" pin="OSCVDD" pad="25"/>
<connect gate="A" pin="OSCVSS" pad="22"/>
<connect gate="A" pin="PLLHV" pad="27"/>
<connect gate="A" pin="RESET" pad="14"/>
<connect gate="A" pin="SPI0_CLK/I2C0_SCL" pad="108"/>
<connect gate="A" pin="SPI0_ENA/I2C1_SDA" pad="105"/>
<connect gate="A" pin="SPI0_SCS/I2C1_SCL" pad="107"/>
<connect gate="A" pin="SPI0_SIMO" pad="110"/>
<connect gate="A" pin="SPI0_SOMI/I2C0_SDA" pad="111"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="28"/>
<connect gate="A" pin="TDO" pad="29"/>
<connect gate="A" pin="TMS" pad="19"/>
<connect gate="A" pin="TRST" pad="21"/>
<connect gate="CVDD" pin="CVDD" pad="8"/>
<connect gate="CVDD" pin="CVDD@1" pad="16"/>
<connect gate="CVDD" pin="CVDD@10" pad="90"/>
<connect gate="CVDD" pin="CVDD@11" pad="101"/>
<connect gate="CVDD" pin="CVDD@12" pad="123"/>
<connect gate="CVDD" pin="CVDD@13" pad="128"/>
<connect gate="CVDD" pin="CVDD@14" pad="132"/>
<connect gate="CVDD" pin="CVDD@2" pad="20"/>
<connect gate="CVDD" pin="CVDD@3" pad="33"/>
<connect gate="CVDD" pin="CVDD@4" pad="44"/>
<connect gate="CVDD" pin="CVDD@5" pad="53"/>
<connect gate="CVDD" pin="CVDD@6" pad="57"/>
<connect gate="CVDD" pin="CVDD@7" pad="65"/>
<connect gate="CVDD" pin="CVDD@8" pad="77"/>
<connect gate="CVDD" pin="CVDD@9" pad="85"/>
<connect gate="DVDD" pin="DVDD" pad="10"/>
<connect gate="DVDD" pin="DVDD@1" pad="31"/>
<connect gate="DVDD" pin="DVDD@10" pad="112"/>
<connect gate="DVDD" pin="DVDD@11" pad="125"/>
<connect gate="DVDD" pin="DVDD@12" pad="136"/>
<connect gate="DVDD" pin="DVDD@2" pad="42"/>
<connect gate="DVDD" pin="DVDD@3" pad="50"/>
<connect gate="DVDD" pin="DVDD@4" pad="60"/>
<connect gate="DVDD" pin="DVDD@5" pad="68"/>
<connect gate="DVDD" pin="DVDD@6" pad="73"/>
<connect gate="DVDD" pin="DVDD@7" pad="81"/>
<connect gate="DVDD" pin="DVDD@8" pad="92"/>
<connect gate="DVDD" pin="DVDD@9" pad="103"/>
<connect gate="EM" pin="EM_A0" pad="91"/>
<connect gate="EM" pin="EM_A1" pad="89"/>
<connect gate="EM" pin="EM_A10" pad="93"/>
<connect gate="EM" pin="EM_A11" pad="74"/>
<connect gate="EM" pin="EM_A2" pad="88"/>
<connect gate="EM" pin="EM_A3" pad="86"/>
<connect gate="EM" pin="EM_A4" pad="84"/>
<connect gate="EM" pin="EM_A5" pad="83"/>
<connect gate="EM" pin="EM_A6" pad="80"/>
<connect gate="EM" pin="EM_A7" pad="79"/>
<connect gate="EM" pin="EM_A8" pad="76"/>
<connect gate="EM" pin="EM_A9" pad="75"/>
<connect gate="EM" pin="EM_BA0" pad="96"/>
<connect gate="EM" pin="EM_BA1" pad="94"/>
<connect gate="EM" pin="EM_CAS" pad="37"/>
<connect gate="EM" pin="EM_CKE" pad="71"/>
<connect gate="EM" pin="EM_CLK" pad="70"/>
<connect gate="EM" pin="EM_CS0" pad="97"/>
<connect gate="EM" pin="EM_CS2" pad="100"/>
<connect gate="EM" pin="EM_D0" pad="52"/>
<connect gate="EM" pin="EM_D1" pad="51"/>
<connect gate="EM" pin="EM_D10" pad="63"/>
<connect gate="EM" pin="EM_D11" pad="61"/>
<connect gate="EM" pin="EM_D12" pad="59"/>
<connect gate="EM" pin="EM_D13" pad="58"/>
<connect gate="EM" pin="EM_D14" pad="56"/>
<connect gate="EM" pin="EM_D15" pad="55"/>
<connect gate="EM" pin="EM_D2" pad="49"/>
<connect gate="EM" pin="EM_D3" pad="48"/>
<connect gate="EM" pin="EM_D4" pad="46"/>
<connect gate="EM" pin="EM_D5" pad="45"/>
<connect gate="EM" pin="EM_D6" pad="43"/>
<connect gate="EM" pin="EM_D7" pad="41"/>
<connect gate="EM" pin="EM_D8" pad="66"/>
<connect gate="EM" pin="EM_D9" pad="64"/>
<connect gate="EM" pin="EM_OE" pad="104"/>
<connect gate="EM" pin="EM_RAS" pad="98"/>
<connect gate="EM" pin="EM_RW" pad="102"/>
<connect gate="EM" pin="EM_WE" pad="38"/>
<connect gate="EM" pin="EM_WE_DQM0" pad="39"/>
<connect gate="EM" pin="EM_WE_DQM1" pad="67"/>
<connect gate="EXP" pin="EXP@1" pad="EXP@1"/>
<connect gate="EXP" pin="EXP@10" pad="EXP@10"/>
<connect gate="EXP" pin="EXP@100" pad="EXP@100"/>
<connect gate="EXP" pin="EXP@11" pad="EXP@11"/>
<connect gate="EXP" pin="EXP@12" pad="EXP@12"/>
<connect gate="EXP" pin="EXP@13" pad="EXP@13"/>
<connect gate="EXP" pin="EXP@14" pad="EXP@14"/>
<connect gate="EXP" pin="EXP@15" pad="EXP@15"/>
<connect gate="EXP" pin="EXP@16" pad="EXP@16"/>
<connect gate="EXP" pin="EXP@17" pad="EXP@17"/>
<connect gate="EXP" pin="EXP@18" pad="EXP@18"/>
<connect gate="EXP" pin="EXP@19" pad="EXP@19"/>
<connect gate="EXP" pin="EXP@2" pad="EXP@2"/>
<connect gate="EXP" pin="EXP@20" pad="EXP@20"/>
<connect gate="EXP" pin="EXP@21" pad="EXP@21"/>
<connect gate="EXP" pin="EXP@22" pad="EXP@22"/>
<connect gate="EXP" pin="EXP@23" pad="EXP@23"/>
<connect gate="EXP" pin="EXP@24" pad="EXP@24"/>
<connect gate="EXP" pin="EXP@25" pad="EXP@25"/>
<connect gate="EXP" pin="EXP@26" pad="EXP@26"/>
<connect gate="EXP" pin="EXP@27" pad="EXP@27"/>
<connect gate="EXP" pin="EXP@28" pad="EXP@28"/>
<connect gate="EXP" pin="EXP@29" pad="EXP@29"/>
<connect gate="EXP" pin="EXP@3" pad="EXP@3"/>
<connect gate="EXP" pin="EXP@30" pad="EXP@30"/>
<connect gate="EXP" pin="EXP@31" pad="EXP@31"/>
<connect gate="EXP" pin="EXP@32" pad="EXP@32"/>
<connect gate="EXP" pin="EXP@33" pad="EXP@33"/>
<connect gate="EXP" pin="EXP@34" pad="EXP@34"/>
<connect gate="EXP" pin="EXP@35" pad="EXP@35"/>
<connect gate="EXP" pin="EXP@36" pad="EXP@36"/>
<connect gate="EXP" pin="EXP@37" pad="EXP@37"/>
<connect gate="EXP" pin="EXP@38" pad="EXP@38"/>
<connect gate="EXP" pin="EXP@39" pad="EXP@39"/>
<connect gate="EXP" pin="EXP@4" pad="EXP@4"/>
<connect gate="EXP" pin="EXP@40" pad="EXP@40"/>
<connect gate="EXP" pin="EXP@41" pad="EXP@41"/>
<connect gate="EXP" pin="EXP@42" pad="EXP@42"/>
<connect gate="EXP" pin="EXP@43" pad="EXP@43"/>
<connect gate="EXP" pin="EXP@44" pad="EXP@44"/>
<connect gate="EXP" pin="EXP@45" pad="EXP@45"/>
<connect gate="EXP" pin="EXP@46" pad="EXP@46"/>
<connect gate="EXP" pin="EXP@47" pad="EXP@47"/>
<connect gate="EXP" pin="EXP@48" pad="EXP@48"/>
<connect gate="EXP" pin="EXP@49" pad="EXP@49"/>
<connect gate="EXP" pin="EXP@5" pad="EXP@5"/>
<connect gate="EXP" pin="EXP@50" pad="EXP@50"/>
<connect gate="EXP" pin="EXP@51" pad="EXP@51"/>
<connect gate="EXP" pin="EXP@52" pad="EXP@52"/>
<connect gate="EXP" pin="EXP@53" pad="EXP@53"/>
<connect gate="EXP" pin="EXP@54" pad="EXP@54"/>
<connect gate="EXP" pin="EXP@55" pad="EXP@55"/>
<connect gate="EXP" pin="EXP@56" pad="EXP@56"/>
<connect gate="EXP" pin="EXP@57" pad="EXP@57"/>
<connect gate="EXP" pin="EXP@58" pad="EXP@58"/>
<connect gate="EXP" pin="EXP@59" pad="EXP@59"/>
<connect gate="EXP" pin="EXP@6" pad="EXP@6"/>
<connect gate="EXP" pin="EXP@60" pad="EXP@60"/>
<connect gate="EXP" pin="EXP@61" pad="EXP@61"/>
<connect gate="EXP" pin="EXP@62" pad="EXP@62"/>
<connect gate="EXP" pin="EXP@63" pad="EXP@63"/>
<connect gate="EXP" pin="EXP@64" pad="EXP@64"/>
<connect gate="EXP" pin="EXP@65" pad="EXP@65"/>
<connect gate="EXP" pin="EXP@66" pad="EXP@66"/>
<connect gate="EXP" pin="EXP@67" pad="EXP@67"/>
<connect gate="EXP" pin="EXP@68" pad="EXP@68"/>
<connect gate="EXP" pin="EXP@69" pad="EXP@69"/>
<connect gate="EXP" pin="EXP@7" pad="EXP@7"/>
<connect gate="EXP" pin="EXP@70" pad="EXP@70"/>
<connect gate="EXP" pin="EXP@71" pad="EXP@71"/>
<connect gate="EXP" pin="EXP@72" pad="EXP@72"/>
<connect gate="EXP" pin="EXP@73" pad="EXP@73"/>
<connect gate="EXP" pin="EXP@74" pad="EXP@74"/>
<connect gate="EXP" pin="EXP@75" pad="EXP@75"/>
<connect gate="EXP" pin="EXP@76" pad="EXP@76"/>
<connect gate="EXP" pin="EXP@77" pad="EXP@77"/>
<connect gate="EXP" pin="EXP@78" pad="EXP@78"/>
<connect gate="EXP" pin="EXP@79" pad="EXP@79"/>
<connect gate="EXP" pin="EXP@8" pad="EXP@8"/>
<connect gate="EXP" pin="EXP@80" pad="EXP@80"/>
<connect gate="EXP" pin="EXP@81" pad="EXP@81"/>
<connect gate="EXP" pin="EXP@82" pad="EXP@82"/>
<connect gate="EXP" pin="EXP@83" pad="EXP@83"/>
<connect gate="EXP" pin="EXP@84" pad="EXP@84"/>
<connect gate="EXP" pin="EXP@85" pad="EXP@85"/>
<connect gate="EXP" pin="EXP@86" pad="EXP@86"/>
<connect gate="EXP" pin="EXP@87" pad="EXP@87"/>
<connect gate="EXP" pin="EXP@88" pad="EXP@88"/>
<connect gate="EXP" pin="EXP@89" pad="EXP@89"/>
<connect gate="EXP" pin="EXP@9" pad="EXP@9"/>
<connect gate="EXP" pin="EXP@90" pad="EXP@90"/>
<connect gate="EXP" pin="EXP@91" pad="EXP@91"/>
<connect gate="EXP" pin="EXP@92" pad="EXP@92"/>
<connect gate="EXP" pin="EXP@93" pad="EXP@93"/>
<connect gate="EXP" pin="EXP@94" pad="EXP@94"/>
<connect gate="EXP" pin="EXP@95" pad="EXP@95"/>
<connect gate="EXP" pin="EXP@96" pad="EXP@96"/>
<connect gate="EXP" pin="EXP@97" pad="EXP@97"/>
<connect gate="EXP" pin="EXP@98" pad="EXP@98"/>
<connect gate="EXP" pin="EXP@99" pad="EXP@99"/>
<connect gate="VSS" pin="VSS" pad="1"/>
<connect gate="VSS" pin="VSS@1" pad="6"/>
<connect gate="VSS" pin="VSS@10" pad="54"/>
<connect gate="VSS" pin="VSS@11" pad="62"/>
<connect gate="VSS" pin="VSS@12" pad="69"/>
<connect gate="VSS" pin="VSS@13" pad="72"/>
<connect gate="VSS" pin="VSS@14" pad="78"/>
<connect gate="VSS" pin="VSS@15" pad="82"/>
<connect gate="VSS" pin="VSS@16" pad="87"/>
<connect gate="VSS" pin="VSS@17" pad="95"/>
<connect gate="VSS" pin="VSS@18" pad="99"/>
<connect gate="VSS" pin="VSS@19" pad="106"/>
<connect gate="VSS" pin="VSS@2" pad="13"/>
<connect gate="VSS" pin="VSS@20" pad="109"/>
<connect gate="VSS" pin="VSS@21" pad="114"/>
<connect gate="VSS" pin="VSS@22" pad="118"/>
<connect gate="VSS" pin="VSS@23" pad="124"/>
<connect gate="VSS" pin="VSS@24" pad="129"/>
<connect gate="VSS" pin="VSS@25" pad="133"/>
<connect gate="VSS" pin="VSS@26" pad="140"/>
<connect gate="VSS" pin="VSS@3" pad="15"/>
<connect gate="VSS" pin="VSS@4" pad="18"/>
<connect gate="VSS" pin="VSS@5" pad="26"/>
<connect gate="VSS" pin="VSS@6" pad="30"/>
<connect gate="VSS" pin="VSS@7" pad="36"/>
<connect gate="VSS" pin="VSS@8" pad="40"/>
<connect gate="VSS" pin="VSS@9" pad="47"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320C6720RFP" prefix="IC">
<description>&lt;b&gt;Floating-Point Digital Signal Processors&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tms320c6720.pdf&lt;br&gt;</description>
<gates>
<gate name="A" symbol="TMS320C6720-QFP-A"/>
<gate name="EM" symbol="TMS320C6720-QFP-EM"/>
<gate name="CVDD" symbol="TMS320C6720-QFP-CVDD"/>
<gate name="DVDD" symbol="TMS320C6720-QFP-DVDD"/>
<gate name="VSS" symbol="TMS320C6720-QFP-VSS"/>
<gate name="EXP" symbol="EXP1"/>
</gates>
<devices>
<device name="" package="RFP_S-PQFP-G144-EXP">
<connects>
<connect gate="A" pin="ACLKR0" pad="139"/>
<connect gate="A" pin="ACLKR1" pad="9"/>
<connect gate="A" pin="ACLKX0" pad="142"/>
<connect gate="A" pin="ACLKX1" pad="7"/>
<connect gate="A" pin="AFSR0" pad="141"/>
<connect gate="A" pin="AFSR1" pad="12"/>
<connect gate="A" pin="AFSX0" pad="144"/>
<connect gate="A" pin="AFSX1" pad="11"/>
<connect gate="A" pin="AHCLKR0/AHCLKR1" pad="143"/>
<connect gate="A" pin="AHCLKX0/AHCLKX2" pad="2"/>
<connect gate="A" pin="AHCLKX1" pad="5"/>
<connect gate="A" pin="AMUTE0" pad="3"/>
<connect gate="A" pin="AMUTE1" pad="4"/>
<connect gate="A" pin="AXR00" pad="113"/>
<connect gate="A" pin="AXR01" pad="115"/>
<connect gate="A" pin="AXR010/AXR13" pad="130"/>
<connect gate="A" pin="AXR011/AXR12" pad="131"/>
<connect gate="A" pin="AXR012/AXR11" pad="134"/>
<connect gate="A" pin="AXR013/AXR10" pad="135"/>
<connect gate="A" pin="AXR014/AXR21" pad="137"/>
<connect gate="A" pin="AXR015/AXR20" pad="138"/>
<connect gate="A" pin="AXR02" pad="116"/>
<connect gate="A" pin="AXR03" pad="117"/>
<connect gate="A" pin="AXR04" pad="119"/>
<connect gate="A" pin="AXR05/SPI1_SCS" pad="120"/>
<connect gate="A" pin="AXR06/SPI1_ENA" pad="121"/>
<connect gate="A" pin="AXR07/SPI1_CLK" pad="122"/>
<connect gate="A" pin="AXR08/AXR15/SPI1_SOMI" pad="126"/>
<connect gate="A" pin="AXR09/AXR14/SPI1_SIMO" pad="127"/>
<connect gate="A" pin="CLKIN" pad="17"/>
<connect gate="A" pin="EMU0" pad="32"/>
<connect gate="A" pin="EMU1" pad="34"/>
<connect gate="A" pin="OSCIN" pad="23"/>
<connect gate="A" pin="OSCOUT" pad="24"/>
<connect gate="A" pin="OSCVDD" pad="25"/>
<connect gate="A" pin="OSCVSS" pad="22"/>
<connect gate="A" pin="PLLHV" pad="27"/>
<connect gate="A" pin="RESET" pad="14"/>
<connect gate="A" pin="SPI0_CLK/I2C0_SCL" pad="108"/>
<connect gate="A" pin="SPI0_ENA/I2C1_SDA" pad="105"/>
<connect gate="A" pin="SPI0_SCS/I2C1_SCL" pad="107"/>
<connect gate="A" pin="SPI0_SIMO" pad="110"/>
<connect gate="A" pin="SPI0_SOMI/I2C0_SDA" pad="111"/>
<connect gate="A" pin="TCK" pad="35"/>
<connect gate="A" pin="TDI" pad="28"/>
<connect gate="A" pin="TDO" pad="29"/>
<connect gate="A" pin="TMS" pad="19"/>
<connect gate="A" pin="TRST" pad="21"/>
<connect gate="CVDD" pin="CVDD" pad="8"/>
<connect gate="CVDD" pin="CVDD@1" pad="16"/>
<connect gate="CVDD" pin="CVDD@10" pad="90"/>
<connect gate="CVDD" pin="CVDD@11" pad="101"/>
<connect gate="CVDD" pin="CVDD@12" pad="123"/>
<connect gate="CVDD" pin="CVDD@13" pad="128"/>
<connect gate="CVDD" pin="CVDD@14" pad="132"/>
<connect gate="CVDD" pin="CVDD@2" pad="20"/>
<connect gate="CVDD" pin="CVDD@3" pad="33"/>
<connect gate="CVDD" pin="CVDD@4" pad="44"/>
<connect gate="CVDD" pin="CVDD@5" pad="53"/>
<connect gate="CVDD" pin="CVDD@6" pad="57"/>
<connect gate="CVDD" pin="CVDD@7" pad="65"/>
<connect gate="CVDD" pin="CVDD@8" pad="77"/>
<connect gate="CVDD" pin="CVDD@9" pad="85"/>
<connect gate="DVDD" pin="DVDD" pad="10"/>
<connect gate="DVDD" pin="DVDD@1" pad="31"/>
<connect gate="DVDD" pin="DVDD@10" pad="112"/>
<connect gate="DVDD" pin="DVDD@11" pad="125"/>
<connect gate="DVDD" pin="DVDD@12" pad="136"/>
<connect gate="DVDD" pin="DVDD@2" pad="42"/>
<connect gate="DVDD" pin="DVDD@3" pad="50"/>
<connect gate="DVDD" pin="DVDD@4" pad="60"/>
<connect gate="DVDD" pin="DVDD@5" pad="68"/>
<connect gate="DVDD" pin="DVDD@6" pad="73"/>
<connect gate="DVDD" pin="DVDD@7" pad="81"/>
<connect gate="DVDD" pin="DVDD@8" pad="92"/>
<connect gate="DVDD" pin="DVDD@9" pad="103"/>
<connect gate="EM" pin="EM_A0" pad="91"/>
<connect gate="EM" pin="EM_A1" pad="89"/>
<connect gate="EM" pin="EM_A10" pad="93"/>
<connect gate="EM" pin="EM_A11" pad="74"/>
<connect gate="EM" pin="EM_A2" pad="88"/>
<connect gate="EM" pin="EM_A3" pad="86"/>
<connect gate="EM" pin="EM_A4" pad="84"/>
<connect gate="EM" pin="EM_A5" pad="83"/>
<connect gate="EM" pin="EM_A6" pad="80"/>
<connect gate="EM" pin="EM_A7" pad="79"/>
<connect gate="EM" pin="EM_A8" pad="76"/>
<connect gate="EM" pin="EM_A9" pad="75"/>
<connect gate="EM" pin="EM_BA0" pad="96"/>
<connect gate="EM" pin="EM_BA1" pad="94"/>
<connect gate="EM" pin="EM_CAS" pad="37"/>
<connect gate="EM" pin="EM_CKE" pad="71"/>
<connect gate="EM" pin="EM_CLK" pad="70"/>
<connect gate="EM" pin="EM_CS0" pad="97"/>
<connect gate="EM" pin="EM_CS2" pad="100"/>
<connect gate="EM" pin="EM_D0" pad="52"/>
<connect gate="EM" pin="EM_D1" pad="51"/>
<connect gate="EM" pin="EM_D10" pad="63"/>
<connect gate="EM" pin="EM_D11" pad="61"/>
<connect gate="EM" pin="EM_D12" pad="59"/>
<connect gate="EM" pin="EM_D13" pad="58"/>
<connect gate="EM" pin="EM_D14" pad="56"/>
<connect gate="EM" pin="EM_D15" pad="55"/>
<connect gate="EM" pin="EM_D2" pad="49"/>
<connect gate="EM" pin="EM_D3" pad="48"/>
<connect gate="EM" pin="EM_D4" pad="46"/>
<connect gate="EM" pin="EM_D5" pad="45"/>
<connect gate="EM" pin="EM_D6" pad="43"/>
<connect gate="EM" pin="EM_D7" pad="41"/>
<connect gate="EM" pin="EM_D8" pad="66"/>
<connect gate="EM" pin="EM_D9" pad="64"/>
<connect gate="EM" pin="EM_OE" pad="104"/>
<connect gate="EM" pin="EM_RAS" pad="98"/>
<connect gate="EM" pin="EM_RW" pad="102"/>
<connect gate="EM" pin="EM_WE" pad="38"/>
<connect gate="EM" pin="EM_WE_DQM0" pad="39"/>
<connect gate="EM" pin="EM_WE_DQM1" pad="67"/>
<connect gate="EXP" pin="EXP" pad="EXP"/>
<connect gate="VSS" pin="VSS" pad="1"/>
<connect gate="VSS" pin="VSS@1" pad="6"/>
<connect gate="VSS" pin="VSS@10" pad="54"/>
<connect gate="VSS" pin="VSS@11" pad="62"/>
<connect gate="VSS" pin="VSS@12" pad="69"/>
<connect gate="VSS" pin="VSS@13" pad="72"/>
<connect gate="VSS" pin="VSS@14" pad="78"/>
<connect gate="VSS" pin="VSS@15" pad="82"/>
<connect gate="VSS" pin="VSS@16" pad="87"/>
<connect gate="VSS" pin="VSS@17" pad="95"/>
<connect gate="VSS" pin="VSS@18" pad="99"/>
<connect gate="VSS" pin="VSS@19" pad="106"/>
<connect gate="VSS" pin="VSS@2" pad="13"/>
<connect gate="VSS" pin="VSS@20" pad="109"/>
<connect gate="VSS" pin="VSS@21" pad="114"/>
<connect gate="VSS" pin="VSS@22" pad="118"/>
<connect gate="VSS" pin="VSS@23" pad="124"/>
<connect gate="VSS" pin="VSS@24" pad="129"/>
<connect gate="VSS" pin="VSS@25" pad="133"/>
<connect gate="VSS" pin="VSS@26" pad="140"/>
<connect gate="VSS" pin="VSS@3" pad="15"/>
<connect gate="VSS" pin="VSS@4" pad="18"/>
<connect gate="VSS" pin="VSS@5" pad="26"/>
<connect gate="VSS" pin="VSS@6" pad="30"/>
<connect gate="VSS" pin="VSS@7" pad="36"/>
<connect gate="VSS" pin="VSS@8" pad="40"/>
<connect gate="VSS" pin="VSS@9" pad="47"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TMS320C6720BRFP200"/>
<attribute name="OC_FARNELL" value="1555284"/>
<attribute name="OC_NEWARK" value="30M1816"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIX4192" prefix="IC">
<description>&lt;b&gt;Integrated Digital Audio Interface Receiver and Transmitter&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/dix4192.pdf</description>
<gates>
<gate name="G$1" symbol="DIX4192"/>
</gates>
<devices>
<device name="" package="S-PQFP-G48">
<connects>
<connect gate="G$1" pin="AESOUT" pad="34"/>
<connect gate="G$1" pin="AGND" pad="10"/>
<connect gate="G$1" pin="BCKA" pad="37"/>
<connect gate="G$1" pin="BCKB" pad="48"/>
<connect gate="G$1" pin="BGND" pad="44"/>
<connect gate="G$1" pin="BLS" pad="35"/>
<connect gate="G$1" pin="CCLK/SCL" pad="20"/>
<connect gate="G$1" pin="CDIN/A1" pad="21"/>
<connect gate="G$1" pin="CDOUT/SDA" pad="22"/>
<connect gate="G$1" pin="CPM" pad="18"/>
<connect gate="G$1" pin="CS/A0" pad="19"/>
<connect gate="G$1" pin="DGND1" pad="16"/>
<connect gate="G$1" pin="DGND2" pad="30"/>
<connect gate="G$1" pin="DGND3" pad="43"/>
<connect gate="G$1" pin="GPO1" pad="26"/>
<connect gate="G$1" pin="GPO2" pad="27"/>
<connect gate="G$1" pin="GPO3" pad="28"/>
<connect gate="G$1" pin="GPO4" pad="29"/>
<connect gate="G$1" pin="INT" pad="23"/>
<connect gate="G$1" pin="LOCK" pad="11"/>
<connect gate="G$1" pin="LRCKA" pad="38"/>
<connect gate="G$1" pin="LRCKB" pad="47"/>
<connect gate="G$1" pin="MCLK" pad="25"/>
<connect gate="G$1" pin="NC" pad="14"/>
<connect gate="G$1" pin="NC@1" pad="15"/>
<connect gate="G$1" pin="NC@2" pad="41"/>
<connect gate="G$1" pin="RST" pad="24"/>
<connect gate="G$1" pin="RX1+" pad="1"/>
<connect gate="G$1" pin="RX1-" pad="2"/>
<connect gate="G$1" pin="RX2+" pad="3"/>
<connect gate="G$1" pin="RX2-" pad="4"/>
<connect gate="G$1" pin="RX3+" pad="5"/>
<connect gate="G$1" pin="RX3-" pad="6"/>
<connect gate="G$1" pin="RX4+" pad="7"/>
<connect gate="G$1" pin="RX4-" pad="8"/>
<connect gate="G$1" pin="RXCKI" pad="13"/>
<connect gate="G$1" pin="RXCKO" pad="12"/>
<connect gate="G$1" pin="SDINA" pad="39"/>
<connect gate="G$1" pin="SDINB" pad="46"/>
<connect gate="G$1" pin="SDOUTA" pad="40"/>
<connect gate="G$1" pin="SDOUTB" pad="45"/>
<connect gate="G$1" pin="SYNC" pad="36"/>
<connect gate="G$1" pin="TX+" pad="32"/>
<connect gate="G$1" pin="TX" pad="31"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VDD18" pad="17"/>
<connect gate="G$1" pin="VDD33" pad="33"/>
<connect gate="G$1" pin="VIO" pad="42"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DIX4192IPFBG4"/>
<attribute name="OC_FARNELL" value="1390700"/>
<attribute name="OC_NEWARK" value="61M5849"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1278" prefix="IC">
<description>&lt;b&gt;Quad/Octal, Simultaneous Sampling, 24-Bit Analog-to-Digital Converters&lt;/b&gt; ADS1274 / ADS1278 &lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1274.pdf</description>
<gates>
<gate name="G$1" symbol="ADS1278"/>
<gate name="P" symbol="EXP25"/>
</gates>
<devices>
<device name="" package="HTQFP-64-PAP">
<connects>
<connect gate="G$1" pin="!DRDY!/FSYNC" pad="29"/>
<connect gate="G$1" pin="!PWDN1" pad="42"/>
<connect gate="G$1" pin="!PWDN2" pad="41"/>
<connect gate="G$1" pin="!PWDN3" pad="40"/>
<connect gate="G$1" pin="!PWDN4" pad="39"/>
<connect gate="G$1" pin="!PWDN5" pad="38"/>
<connect gate="G$1" pin="!PWDN6" pad="37"/>
<connect gate="G$1" pin="!PWDN7" pad="36"/>
<connect gate="G$1" pin="!PWDN8" pad="35"/>
<connect gate="G$1" pin="!SYNC" pad="11"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AGND@1" pad="43"/>
<connect gate="G$1" pin="AGND@2" pad="54"/>
<connect gate="G$1" pin="AGND@3" pad="58"/>
<connect gate="G$1" pin="AGND@4" pad="59"/>
<connect gate="G$1" pin="AINN1" pad="4"/>
<connect gate="G$1" pin="AINN2" pad="2"/>
<connect gate="G$1" pin="AINN3" pad="64"/>
<connect gate="G$1" pin="AINN4" pad="62"/>
<connect gate="G$1" pin="AINN5" pad="52"/>
<connect gate="G$1" pin="AINN6" pad="50"/>
<connect gate="G$1" pin="AINN7" pad="48"/>
<connect gate="G$1" pin="AINN8" pad="46"/>
<connect gate="G$1" pin="AINP1" pad="3"/>
<connect gate="G$1" pin="AINP2" pad="1"/>
<connect gate="G$1" pin="AINP3" pad="63"/>
<connect gate="G$1" pin="AINP4" pad="61"/>
<connect gate="G$1" pin="AINP5" pad="51"/>
<connect gate="G$1" pin="AINP6" pad="49"/>
<connect gate="G$1" pin="AINP7" pad="47"/>
<connect gate="G$1" pin="AINP8" pad="45"/>
<connect gate="G$1" pin="AVDD" pad="5"/>
<connect gate="G$1" pin="AVDD@1" pad="44"/>
<connect gate="G$1" pin="AVDD@2" pad="53"/>
<connect gate="G$1" pin="AVDD@3" pad="60"/>
<connect gate="G$1" pin="CLK" pad="27"/>
<connect gate="G$1" pin="CLKDIV" pad="10"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DGND@1" pad="21"/>
<connect gate="G$1" pin="DGND@2" pad="24"/>
<connect gate="G$1" pin="DGND@3" pad="25"/>
<connect gate="G$1" pin="DIN" pad="12"/>
<connect gate="G$1" pin="DOUT1" pad="20"/>
<connect gate="G$1" pin="DOUT2" pad="19"/>
<connect gate="G$1" pin="DOUT3" pad="18"/>
<connect gate="G$1" pin="DOUT4" pad="17"/>
<connect gate="G$1" pin="DOUT5" pad="16"/>
<connect gate="G$1" pin="DOUT6" pad="15"/>
<connect gate="G$1" pin="DOUT7" pad="14"/>
<connect gate="G$1" pin="DOUT8" pad="13"/>
<connect gate="G$1" pin="DVDD" pad="26"/>
<connect gate="G$1" pin="FORMAT0" pad="32"/>
<connect gate="G$1" pin="FORMAT1" pad="31"/>
<connect gate="G$1" pin="FORMAT2" pad="30"/>
<connect gate="G$1" pin="IOVDD" pad="22"/>
<connect gate="G$1" pin="IOVDD@1" pad="23"/>
<connect gate="G$1" pin="MODE0" pad="34"/>
<connect gate="G$1" pin="MODE1" pad="33"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="TEST0" pad="8"/>
<connect gate="G$1" pin="TEST1" pad="9"/>
<connect gate="G$1" pin="VCOM" pad="55"/>
<connect gate="G$1" pin="VREFN" pad="57"/>
<connect gate="G$1" pin="VREFP" pad="56"/>
<connect gate="P" pin="EXP@1" pad="EXP1"/>
<connect gate="P" pin="EXP@10" pad="EXP10"/>
<connect gate="P" pin="EXP@11" pad="EXP11"/>
<connect gate="P" pin="EXP@12" pad="EXP12"/>
<connect gate="P" pin="EXP@13" pad="EXP13"/>
<connect gate="P" pin="EXP@14" pad="EXP14"/>
<connect gate="P" pin="EXP@15" pad="EXP15"/>
<connect gate="P" pin="EXP@16" pad="EXP16"/>
<connect gate="P" pin="EXP@17" pad="EXP17"/>
<connect gate="P" pin="EXP@18" pad="EXP18"/>
<connect gate="P" pin="EXP@19" pad="EXP19"/>
<connect gate="P" pin="EXP@2" pad="EXP2"/>
<connect gate="P" pin="EXP@20" pad="EXP20"/>
<connect gate="P" pin="EXP@21" pad="EXP21"/>
<connect gate="P" pin="EXP@22" pad="EXP22"/>
<connect gate="P" pin="EXP@23" pad="EXP23"/>
<connect gate="P" pin="EXP@24" pad="EXP24"/>
<connect gate="P" pin="EXP@25" pad="EXP25"/>
<connect gate="P" pin="EXP@3" pad="EXP3"/>
<connect gate="P" pin="EXP@4" pad="EXP4"/>
<connect gate="P" pin="EXP@5" pad="EXP5"/>
<connect gate="P" pin="EXP@6" pad="EXP6"/>
<connect gate="P" pin="EXP@7" pad="EXP7"/>
<connect gate="P" pin="EXP@8" pad="EXP8"/>
<connect gate="P" pin="EXP@9" pad="EXP9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS1278IPAPT"/>
<attribute name="OC_FARNELL" value="1603419"/>
<attribute name="OC_NEWARK" value="50M8811"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1271" prefix="IC">
<description>&lt;b&gt;24-Bit Wide Bandwidth Analaog-to-Digial Converter&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1271.pdf</description>
<gates>
<gate name="G$1" symbol="ADS1271"/>
</gates>
<devices>
<device name="" package="TSSOP16">
<connects>
<connect gate="G$1" pin="!DRDY!/FSYNC" pad="10"/>
<connect gate="G$1" pin="!SYNC!/!PDWN" pad="7"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AINN" pad="2"/>
<connect gate="G$1" pin="AINP" pad="1"/>
<connect gate="G$1" pin="AVDD" pad="4"/>
<connect gate="G$1" pin="CLK" pad="12"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DIN" pad="8"/>
<connect gate="G$1" pin="DOUT" pad="9"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="FORMAT" pad="6"/>
<connect gate="G$1" pin="MODE" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="VREFN" pad="15"/>
<connect gate="G$1" pin="VREFP" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS1271IPWR"/>
<attribute name="OC_FARNELL" value="9968865"/>
<attribute name="OC_NEWARK" value="73J8186"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO1050" prefix="IC">
<description>&lt;b&gt;ISOLATED CAN TRANSCEIVER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/iso1050.pdf</description>
<gates>
<gate name="G$1" symbol="ISO1050"/>
</gates>
<devices>
<device name="DUB" package="DUB-R-PDSO-G8">
<connects>
<connect gate="G$1" pin="CANH" pad="7"/>
<connect gate="G$1" pin="CANL" pad="6"/>
<connect gate="G$1" pin="GND1" pad="4"/>
<connect gate="G$1" pin="GND2" pad="5"/>
<connect gate="G$1" pin="RXD" pad="2"/>
<connect gate="G$1" pin="TXD" pad="3"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO1050DUBR"/>
<attribute name="OC_FARNELL" value="1755712"/>
<attribute name="OC_NEWARK" value="14R9899"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1210" prefix="IC">
<description>&lt;b&gt;24-Bit ANALOG-TO-DIGITAL CONVERTER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1210.pdf</description>
<gates>
<gate name="G$1" symbol="ADS1210"/>
</gates>
<devices>
<device name="P" package="DIL18">
<connects>
<connect gate="G$1" pin="!DRDY" pad="14"/>
<connect gate="G$1" pin="!DSYNC" pad="6"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AINN" pad="2"/>
<connect gate="G$1" pin="AINP" pad="1"/>
<connect gate="G$1" pin="AVDD" pad="16"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DVDD" pad="10"/>
<connect gate="G$1" pin="MODE" pad="15"/>
<connect gate="G$1" pin="REFIN" pad="18"/>
<connect gate="G$1" pin="REFOUT" pad="17"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDIO" pad="12"/>
<connect gate="G$1" pin="SDOUT" pad="13"/>
<connect gate="G$1" pin="VBIAS" pad="4"/>
<connect gate="G$1" pin="XIN" pad="7"/>
<connect gate="G$1" pin="XOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1210P"/>
<attribute name="OC_FARNELL" value="1312336"/>
<attribute name="OC_NEWARK" value="96K4580"/>
</technology>
</technologies>
</device>
<device name="U" package="SO-18DW">
<connects>
<connect gate="G$1" pin="!DRDY" pad="14"/>
<connect gate="G$1" pin="!DSYNC" pad="6"/>
<connect gate="G$1" pin="AGND" pad="3"/>
<connect gate="G$1" pin="AINN" pad="2"/>
<connect gate="G$1" pin="AINP" pad="1"/>
<connect gate="G$1" pin="AVDD" pad="16"/>
<connect gate="G$1" pin="CS" pad="5"/>
<connect gate="G$1" pin="DGND" pad="9"/>
<connect gate="G$1" pin="DVDD" pad="10"/>
<connect gate="G$1" pin="MODE" pad="15"/>
<connect gate="G$1" pin="REFIN" pad="18"/>
<connect gate="G$1" pin="REFOUT" pad="17"/>
<connect gate="G$1" pin="SCLK" pad="11"/>
<connect gate="G$1" pin="SDIO" pad="12"/>
<connect gate="G$1" pin="SDOUT" pad="13"/>
<connect gate="G$1" pin="VBIAS" pad="4"/>
<connect gate="G$1" pin="XIN" pad="7"/>
<connect gate="G$1" pin="XOUT" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1210U"/>
<attribute name="OC_FARNELL" value="1295983"/>
<attribute name="OC_NEWARK" value="74K3627"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1211" prefix="IC">
<description>&lt;b&gt;24-Bit ANALOG-TO-DIGITAL CONVERTER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1210.pdf</description>
<gates>
<gate name="G$1" symbol="ADS1211"/>
</gates>
<devices>
<device name="U" package="PW_R-PDSO-G24">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="!DRDY" pad="17"/>
<connect gate="G$1" pin="!DSYNC" pad="9"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="24"/>
<connect gate="G$1" pin="AIN4N" pad="23"/>
<connect gate="G$1" pin="AIN4P" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="MODE" pad="18"/>
<connect gate="G$1" pin="REFIN" pad="21"/>
<connect gate="G$1" pin="REFOUT" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="SDIO" pad="15"/>
<connect gate="G$1" pin="SDOUT" pad="16"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="10"/>
<connect gate="G$1" pin="XOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1211U"/>
<attribute name="OC_FARNELL" value="9324070"/>
<attribute name="OC_NEWARK" value="35C1513"/>
</technology>
</technologies>
</device>
<device name="P" package="PDIP-T24">
<connects>
<connect gate="G$1" pin="!CS" pad="8"/>
<connect gate="G$1" pin="!DRDY" pad="17"/>
<connect gate="G$1" pin="!DSYNC" pad="9"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="24"/>
<connect gate="G$1" pin="AIN4N" pad="23"/>
<connect gate="G$1" pin="AIN4P" pad="22"/>
<connect gate="G$1" pin="AVDD" pad="19"/>
<connect gate="G$1" pin="DGND" pad="12"/>
<connect gate="G$1" pin="DVDD" pad="13"/>
<connect gate="G$1" pin="MODE" pad="18"/>
<connect gate="G$1" pin="REFIN" pad="21"/>
<connect gate="G$1" pin="REFOUT" pad="20"/>
<connect gate="G$1" pin="SCLK" pad="14"/>
<connect gate="G$1" pin="SDIO" pad="15"/>
<connect gate="G$1" pin="SDOUT" pad="16"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="10"/>
<connect gate="G$1" pin="XOUT" pad="11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="ADS1211P"/>
<attribute name="OC_FARNELL" value="1219430"/>
<attribute name="OC_NEWARK" value="96K2329"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1211E" prefix="IC">
<description>&lt;b&gt;24-Bit ANALOG-TO-DIGITAL CONVERTER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1210.pdf</description>
<gates>
<gate name="G$1" symbol="ADS1211E"/>
</gates>
<devices>
<device name="" package="DB_R-PDSO-G28">
<connects>
<connect gate="G$1" pin="!CS" pad="10"/>
<connect gate="G$1" pin="!DRDY" pad="19"/>
<connect gate="G$1" pin="!DSYNC" pad="11"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AIN1N" pad="5"/>
<connect gate="G$1" pin="AIN1P" pad="4"/>
<connect gate="G$1" pin="AIN2N" pad="3"/>
<connect gate="G$1" pin="AIN2P" pad="2"/>
<connect gate="G$1" pin="AIN3N" pad="1"/>
<connect gate="G$1" pin="AIN3P" pad="28"/>
<connect gate="G$1" pin="AIN4N" pad="27"/>
<connect gate="G$1" pin="AIN4P" pad="26"/>
<connect gate="G$1" pin="AVDD" pad="23"/>
<connect gate="G$1" pin="DGND" pad="14"/>
<connect gate="G$1" pin="DVDD" pad="15"/>
<connect gate="G$1" pin="MODE" pad="22"/>
<connect gate="G$1" pin="NC" pad="8"/>
<connect gate="G$1" pin="NC@1" pad="9"/>
<connect gate="G$1" pin="NC@2" pad="20"/>
<connect gate="G$1" pin="NC@3" pad="21"/>
<connect gate="G$1" pin="REFIN" pad="25"/>
<connect gate="G$1" pin="REFOUT" pad="24"/>
<connect gate="G$1" pin="SCLK" pad="16"/>
<connect gate="G$1" pin="SDIO" pad="17"/>
<connect gate="G$1" pin="SDOUT" pad="18"/>
<connect gate="G$1" pin="VBIAS" pad="7"/>
<connect gate="G$1" pin="XIN" pad="12"/>
<connect gate="G$1" pin="XOUT" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="ADS1211E"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="74C6976"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OMAP-L137" prefix="IC">
<description>&lt;b&gt;OMAP-L137 Low-Power Applications Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: sprm328.bsm&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/omap-l137.pdf</description>
<gates>
<gate name="A" symbol="OMAP-L137_A"/>
<gate name="B" symbol="OMAP-L137_B"/>
<gate name="C" symbol="OMAP-L137_C"/>
<gate name="D" symbol="OMAP-L137_D"/>
<gate name="P" symbol="OMAP-L137_P"/>
</gates>
<devices>
<device name="" package="ZKB_S-PBGA-N256">
<connects>
<connect gate="A" pin="ACLKR0/ECAP1/APWM1/GP215" pad="B4"/>
<connect gate="A" pin="ACLKR1/ECAP2/APWM2/GP412" pad="L2"/>
<connect gate="A" pin="ACLKX0/ECAP0/APWM0/GP212" pad="C5"/>
<connect gate="A" pin="ACLKX1/EPWM0A/GP315" pad="K3"/>
<connect gate="A" pin="AFSR0/GP312" pad="C4"/>
<connect gate="A" pin="AFSR1/GP413" pad="L3"/>
<connect gate="A" pin="AFSX0/GP213/BOOT10" pad="D5"/>
<connect gate="A" pin="AFSX1/EPWMSYNCI/EPWMSYNCO/GP410" pad="K4"/>
<connect gate="A" pin="AHCLKR0/RMII_MHZ50CLK/GP214/BOOT11" pad="A4"/>
<connect gate="A" pin="AHCLKR1/GP411" pad="L1"/>
<connect gate="A" pin="AHCLKX0/AHCLKX2/USBREFCLKIN/GP211" pad="B5"/>
<connect gate="A" pin="AHCLKX1/EPWM0B/GP314" pad="K2"/>
<connect gate="A" pin="AMUTE0/!RESETOUT" pad="L4"/>
<connect gate="A" pin="AMUTE1/EPWMTZ/GP414" pad="D4"/>
<connect gate="A" pin="AXR00/RMII_TXD0/AFSR2/GP30" pad="B8"/>
<connect gate="A" pin="AXR01/RMII_TXD1/ACLKX2/GP31" pad="C8"/>
<connect gate="A" pin="AXR010/UART1TXD/GP310" pad="D6"/>
<connect gate="A" pin="AXR011/AXR20/GP311" pad="A5"/>
<connect gate="A" pin="AXR02/RMII_TXEN/AXR23/GP32" pad="D8"/>
<connect gate="A" pin="AXR03/RMII_CRSDV/AXR22/GP33" pad="A7"/>
<connect gate="A" pin="AXR04/RMII_RXD0/AXR21/GP34" pad="B7"/>
<connect gate="A" pin="AXR05/RMII_RXD1/AFSX2/GP35" pad="C7"/>
<connect gate="A" pin="AXR06/RMII_RXER/ACLKR2/GP36" pad="D7"/>
<connect gate="A" pin="AXR07/MDIOCLK/GP37" pad="A6"/>
<connect gate="A" pin="AXR08/MDIOD/GP38" pad="B6"/>
<connect gate="A" pin="AXR09/UART1RXD/GP39" pad="C6"/>
<connect gate="A" pin="AXR10/GP40" pad="T3"/>
<connect gate="A" pin="AXR11/GP41" pad="R2"/>
<connect gate="A" pin="AXR110/GP510" pad="N3"/>
<connect gate="A" pin="AXR111/GP511" pad="T4"/>
<connect gate="A" pin="AXR12/GP42" pad="P2"/>
<connect gate="A" pin="AXR13/EQEP1A/GP43" pad="P1"/>
<connect gate="A" pin="AXR14/EQEP1B/GP44" pad="N2"/>
<connect gate="A" pin="AXR15/EPWM2B/GP45" pad="N1"/>
<connect gate="A" pin="AXR16/EPWM2A/GP46" pad="M4"/>
<connect gate="A" pin="AXR17/EPWM1B/GP47" pad="M3"/>
<connect gate="A" pin="AXR18/EPWM1A/GP48" pad="M2"/>
<connect gate="A" pin="AXR19/GP49" pad="M1"/>
<connect gate="B" pin="!EMA_CAS!/!EMA_CS4!/GP21" pad="L16"/>
<connect gate="B" pin="!EMA_CS0!/!UHPIHAS!/GP24" pad="T8"/>
<connect gate="B" pin="!EMA_CS2!/!UHPIHCS!/GP25/BOOT15" pad="P7"/>
<connect gate="B" pin="!EMA_CS3!/AMUTE2/GP26" pad="T7"/>
<connect gate="B" pin="!EMA_OE!/!UHPIHDS1!/AXR013/GP27" pad="R7"/>
<connect gate="B" pin="!EMA_RAS!/!EMA_CS5!/GP22" pad="N7"/>
<connect gate="B" pin="!EMA_WE!/UHPIHR!W!/AXR012/GP23/BOOT14" pad="M13"/>
<connect gate="B" pin="!EMA_WEDQM0!/!UHPIHINT!/AXR015/GP29" pad="M14"/>
<connect gate="B" pin="!EMA_WEDQM1!/!UHPIHDS2!/AXR014/GP28" pad="P12"/>
<connect gate="B" pin="EMA_A0/LCDD7/GP10" pad="T9"/>
<connect gate="B" pin="EMA_A1/MMCSDCLK/UHPIHCNTL0/GP11" pad="R9"/>
<connect gate="B" pin="EMA_A10/LCDVSYNC/GP110" pad="N8"/>
<connect gate="B" pin="EMA_A11/!LCDACENBCS!/GP111" pad="P11"/>
<connect gate="B" pin="EMA_A12/LCDMCLK/GP112" pad="N11"/>
<connect gate="B" pin="EMA_A2/MMCSDCMD/UHPIHCNTL1/GP12" pad="P9"/>
<connect gate="B" pin="EMA_A3/LCDD6/GP13" pad="N9"/>
<connect gate="B" pin="EMA_A4/LCDD3/GP14" pad="T10"/>
<connect gate="B" pin="EMA_A5/LCDD2/GP15" pad="R10"/>
<connect gate="B" pin="EMA_A6/LCDD1/GP16" pad="P10"/>
<connect gate="B" pin="EMA_A7/LCDD0/GP17" pad="N10"/>
<connect gate="B" pin="EMA_A8/LCDPCLK/GP18" pad="T11"/>
<connect gate="B" pin="EMA_A9/LCDHSYNC/GP19" pad="R11"/>
<connect gate="B" pin="EMA_BA0/LCDD4/GP114" pad="R8"/>
<connect gate="B" pin="EMA_BA1/LCDD5/UHPIHHWIL/GP113" pad="P8"/>
<connect gate="B" pin="EMA_CLK/OBSCLK/AHCLKR2/GP115" pad="R12"/>
<connect gate="B" pin="EMA_D0/MMCSDDAT0/UHPIHD0/GP00/BOOT12" pad="T13"/>
<connect gate="B" pin="EMA_D1/MMCSDDAT1/UHPIHD1/GP01" pad="R15"/>
<connect gate="B" pin="EMA_D10/UHPIHD10/LCDD10/GP010" pad="R14"/>
<connect gate="B" pin="EMA_D11/UHPIHD11/LCDD11/GP011" pad="P16"/>
<connect gate="B" pin="EMA_D12/UHPIHD12/LCDD12/GP012" pad="P14"/>
<connect gate="B" pin="EMA_D13/UHPIHD13/LCDD13/GP013" pad="N16"/>
<connect gate="B" pin="EMA_D14/UHPIHD14/LCDD14/GP014" pad="N14"/>
<connect gate="B" pin="EMA_D15/UHPIHD15/LCDD15/GP015" pad="M16"/>
<connect gate="B" pin="EMA_D2/MMCSDDAT2/UHPIHD2/GP02" pad="R13"/>
<connect gate="B" pin="EMA_D3/MMCSDDAT3/UHPIHD3/GP03" pad="P15"/>
<connect gate="B" pin="EMA_D4/MMCSDDAT4/UHPIHD4/GP04" pad="P13"/>
<connect gate="B" pin="EMA_D5/MMCSDDAT5/UHPIHD5/GP05" pad="N15"/>
<connect gate="B" pin="EMA_D6/MMCSDDAT6/UHPIHD6/GP06" pad="N13"/>
<connect gate="B" pin="EMA_D7/MMCSDDAT7/UHPIHD7/GP07/BOOT13" pad="M15"/>
<connect gate="B" pin="EMA_D8/UHPIHD8/LCDD8/GP08" pad="N12"/>
<connect gate="B" pin="EMA_D9/UHPIHD9/LCDD9/GP09" pad="T14"/>
<connect gate="B" pin="EMA_SDCKE/GP20" pad="T12"/>
<connect gate="B" pin="EMA_WAIT0/!UHPIHRDY!/GP210" pad="N6"/>
<connect gate="C" pin="!EMB_CAS" pad="L13"/>
<connect gate="C" pin="!EMB_CS0" pad="D9"/>
<connect gate="C" pin="!EMB_RAS" pad="A8"/>
<connect gate="C" pin="!EMB_WE" pad="K15"/>
<connect gate="C" pin="!EMB_WEDQM0!/GP515" pad="K14"/>
<connect gate="C" pin="!EMB_WEDQM1!/GP514" pad="C15"/>
<connect gate="C" pin="!EMB_WEDQM2!" pad="B13"/>
<connect gate="C" pin="!EMB_WEDQM3!" pad="A12"/>
<connect gate="C" pin="EMB_A0/GP72" pad="D10"/>
<connect gate="C" pin="EMB_A1/GP73" pad="C10"/>
<connect gate="C" pin="EMB_A10/GP712" pad="A9"/>
<connect gate="C" pin="EMB_A11/GP713" pad="B12"/>
<connect gate="C" pin="EMB_A12/GP313" pad="B15"/>
<connect gate="C" pin="EMB_A2/GP74" pad="B10"/>
<connect gate="C" pin="EMB_A3/GP75" pad="A10"/>
<connect gate="C" pin="EMB_A4/GP76" pad="D11"/>
<connect gate="C" pin="EMB_A5/GP77" pad="C11"/>
<connect gate="C" pin="EMB_A6/GP78" pad="B11"/>
<connect gate="C" pin="EMB_A7/GP79" pad="A11"/>
<connect gate="C" pin="EMB_A8/GP710" pad="D12"/>
<connect gate="C" pin="EMB_A9/GP711" pad="C12"/>
<connect gate="C" pin="EMB_BA0/GP71" pad="C9"/>
<connect gate="C" pin="EMB_BA1/GP70" pad="B9"/>
<connect gate="C" pin="EMB_CLK" pad="C14"/>
<connect gate="C" pin="EMB_D0/GP60" pad="F16"/>
<connect gate="C" pin="EMB_D1/GP61" pad="G13"/>
<connect gate="C" pin="EMB_D10/GP610" pad="D14"/>
<connect gate="C" pin="EMB_D11/GP611" pad="D15"/>
<connect gate="C" pin="EMB_D12/GP612" pad="D16"/>
<connect gate="C" pin="EMB_D13/GP613" pad="E13"/>
<connect gate="C" pin="EMB_D14/GP614" pad="E16"/>
<connect gate="C" pin="EMB_D15/GP615" pad="F13"/>
<connect gate="C" pin="EMB_D16" pad="G15"/>
<connect gate="C" pin="EMB_D17" pad="H14"/>
<connect gate="C" pin="EMB_D18" pad="H15"/>
<connect gate="C" pin="EMB_D19" pad="J14"/>
<connect gate="C" pin="EMB_D2/GP62" pad="G16"/>
<connect gate="C" pin="EMB_D20" pad="K13"/>
<connect gate="C" pin="EMB_D21" pad="K16"/>
<connect gate="C" pin="EMB_D22" pad="L14"/>
<connect gate="C" pin="EMB_D23" pad="L15"/>
<connect gate="C" pin="EMB_D24" pad="A13"/>
<connect gate="C" pin="EMB_D25" pad="B14"/>
<connect gate="C" pin="EMB_D26" pad="A14"/>
<connect gate="C" pin="EMB_D27" pad="E14"/>
<connect gate="C" pin="EMB_D28" pad="E15"/>
<connect gate="C" pin="EMB_D29" pad="F14"/>
<connect gate="C" pin="EMB_D3/GP63" pad="H13"/>
<connect gate="C" pin="EMB_D30" pad="F15"/>
<connect gate="C" pin="EMB_D31" pad="G14"/>
<connect gate="C" pin="EMB_D4/GP64" pad="H16"/>
<connect gate="C" pin="EMB_D5/GP65" pad="J13"/>
<connect gate="C" pin="EMB_D6/GP66" pad="J15"/>
<connect gate="C" pin="EMB_D7/GP67" pad="J16"/>
<connect gate="C" pin="EMB_D8/GP68" pad="C16"/>
<connect gate="C" pin="EMB_D9/GP69" pad="D13"/>
<connect gate="C" pin="EMB_SDCKE" pad="C13"/>
<connect gate="D" pin="!RESET" pad="G3"/>
<connect gate="D" pin="!SPI0_ENA!/!UART0CTS!/EQEP0A/GP53/BOOT3" pad="R5"/>
<connect gate="D" pin="!SPI0_SCS0!/!UART0RTS!/EQEP0B/GP54/BOOT4" pad="N4"/>
<connect gate="D" pin="!SPI1_ENA!/UART2RXD/GP512" pad="R4"/>
<connect gate="D" pin="!SPI1_SCS0!/UART2TXD/GP513" pad="P4"/>
<connect gate="D" pin="!TRST" pad="J4"/>
<connect gate="D" pin="EMU0/GP715" pad="J5"/>
<connect gate="D" pin="NC1" pad="F3"/>
<connect gate="D" pin="NC2" pad="H4"/>
<connect gate="D" pin="OSCIN" pad="F2"/>
<connect gate="D" pin="OSCOUT" pad="F1"/>
<connect gate="D" pin="OSCVSS" pad="E2"/>
<connect gate="D" pin="PLL0_VDDA" pad="D1"/>
<connect gate="D" pin="PLL0_VSSA" pad="E1"/>
<connect gate="D" pin="RSV1" pad="F7"/>
<connect gate="D" pin="RSV2" pad="B1"/>
<connect gate="D" pin="RTC/XI" pad="H1"/>
<connect gate="D" pin="RTC/XO" pad="H2"/>
<connect gate="D" pin="RTCK" pad="K1"/>
<connect gate="D" pin="RTC_CVDD" pad="G1"/>
<connect gate="D" pin="RTC_VSS" pad="G2"/>
<connect gate="D" pin="SPI0_CLK/EQEP1I/GP52/BOOT2" pad="T5"/>
<connect gate="D" pin="SPI0_SIMO0/EQEP0S/GP51/BOOT1" pad="P6"/>
<connect gate="D" pin="SPI0_SOMI0/EQEP0I/GP50/BOOT0" pad="R6"/>
<connect gate="D" pin="SPI1_CLK/EQEP1S/GP57/BOOT7" pad="T6"/>
<connect gate="D" pin="SPI1_SIMO0/I2C1SDA/GP56/BOOT6" pad="N5"/>
<connect gate="D" pin="SPI1_SOMI0/I2C1SCL/GP55/BOOT5" pad="P5"/>
<connect gate="D" pin="TCK" pad="H3"/>
<connect gate="D" pin="TDI" pad="J2"/>
<connect gate="D" pin="TDO" pad="J3"/>
<connect gate="D" pin="TMS" pad="J1"/>
<connect gate="D" pin="UART0RXD/I2C0SDA/TM64P0IN12/GP58/BOOT8" pad="R3"/>
<connect gate="D" pin="UART0TXD/I2C0SCL/TM64P0OUT12/GP59/BOOT9" pad="P3"/>
<connect gate="D" pin="USB0/DM" pad="G4"/>
<connect gate="D" pin="USB0/DP" pad="F4"/>
<connect gate="D" pin="USB0/ID" pad="D2"/>
<connect gate="D" pin="USB0/VBUS" pad="D3"/>
<connect gate="D" pin="USB0DRVVBUS/GP415" pad="E4"/>
<connect gate="D" pin="USB1/DM" pad="B3"/>
<connect gate="D" pin="USB1/DP" pad="A3"/>
<connect gate="P" pin="VDD@1" pad="R1"/>
<connect gate="P" pin="VDD@10" pad="L12"/>
<connect gate="P" pin="VDD@11" pad="K5"/>
<connect gate="P" pin="VDD@12" pad="K6"/>
<connect gate="P" pin="VDD@13" pad="K7"/>
<connect gate="P" pin="VDD@14" pad="K10"/>
<connect gate="P" pin="VDD@15" pad="K11"/>
<connect gate="P" pin="VDD@16" pad="K12"/>
<connect gate="P" pin="VDD@17" pad="J6"/>
<connect gate="P" pin="VDD@18" pad="J7"/>
<connect gate="P" pin="VDD@19" pad="J10"/>
<connect gate="P" pin="VDD@2" pad="R16"/>
<connect gate="P" pin="VDD@20" pad="J11"/>
<connect gate="P" pin="VDD@21" pad="J12"/>
<connect gate="P" pin="VDD@22" pad="H5"/>
<connect gate="P" pin="VDD@23" pad="H6"/>
<connect gate="P" pin="VDD@24" pad="H7"/>
<connect gate="P" pin="VDD@25" pad="H10"/>
<connect gate="P" pin="VDD@26" pad="H11"/>
<connect gate="P" pin="VDD@27" pad="H12"/>
<connect gate="P" pin="VDD@29" pad="G5"/>
<connect gate="P" pin="VDD@3" pad="M5"/>
<connect gate="P" pin="VDD@30" pad="G6"/>
<connect gate="P" pin="VDD@31" pad="G7"/>
<connect gate="P" pin="VDD@32" pad="G10"/>
<connect gate="P" pin="VDD@33" pad="G11"/>
<connect gate="P" pin="VDD@34" pad="G12"/>
<connect gate="P" pin="VDD@35" pad="F5"/>
<connect gate="P" pin="VDD@36" pad="F6"/>
<connect gate="P" pin="VDD@37" pad="F11"/>
<connect gate="P" pin="VDD@38" pad="F12"/>
<connect gate="P" pin="VDD@39" pad="E3"/>
<connect gate="P" pin="VDD@4" pad="M8"/>
<connect gate="P" pin="VDD@40" pad="E5"/>
<connect gate="P" pin="VDD@41" pad="E8"/>
<connect gate="P" pin="VDD@42" pad="E9"/>
<connect gate="P" pin="VDD@43" pad="E12"/>
<connect gate="P" pin="VDD@45" pad="C1"/>
<connect gate="P" pin="VDD@46" pad="C2"/>
<connect gate="P" pin="VDD@47" pad="C3"/>
<connect gate="P" pin="VDD@48" pad="B16"/>
<connect gate="P" pin="VDD@5" pad="M9"/>
<connect gate="P" pin="VDD@6" pad="M12"/>
<connect gate="P" pin="VDD@7" pad="L5"/>
<connect gate="P" pin="VDD@8" pad="L6"/>
<connect gate="P" pin="VDD@9" pad="L11"/>
<connect gate="P" pin="VSS@1" pad="T1"/>
<connect gate="P" pin="VSS@10" pad="L8"/>
<connect gate="P" pin="VSS@11" pad="L9"/>
<connect gate="P" pin="VSS@12" pad="L10"/>
<connect gate="P" pin="VSS@13" pad="K8"/>
<connect gate="P" pin="VSS@14" pad="K9"/>
<connect gate="P" pin="VSS@15" pad="J8"/>
<connect gate="P" pin="VSS@16" pad="J9"/>
<connect gate="P" pin="VSS@17" pad="H8"/>
<connect gate="P" pin="VSS@18" pad="H9"/>
<connect gate="P" pin="VSS@2" pad="T2"/>
<connect gate="P" pin="VSS@20" pad="G8"/>
<connect gate="P" pin="VSS@21" pad="G9"/>
<connect gate="P" pin="VSS@22" pad="F8"/>
<connect gate="P" pin="VSS@23" pad="F9"/>
<connect gate="P" pin="VSS@24" pad="F10"/>
<connect gate="P" pin="VSS@27" pad="E6"/>
<connect gate="P" pin="VSS@28" pad="E7"/>
<connect gate="P" pin="VSS@29" pad="E10"/>
<connect gate="P" pin="VSS@3" pad="T15"/>
<connect gate="P" pin="VSS@30" pad="E11"/>
<connect gate="P" pin="VSS@31" pad="B2"/>
<connect gate="P" pin="VSS@32" pad="A1"/>
<connect gate="P" pin="VSS@33" pad="A2"/>
<connect gate="P" pin="VSS@34" pad="A15"/>
<connect gate="P" pin="VSS@35" pad="A16"/>
<connect gate="P" pin="VSS@4" pad="T16"/>
<connect gate="P" pin="VSS@5" pad="M6"/>
<connect gate="P" pin="VSS@6" pad="M7"/>
<connect gate="P" pin="VSS@7" pad="M10"/>
<connect gate="P" pin="VSS@8" pad="M11"/>
<connect gate="P" pin="VSS@9" pad="L7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="OMAP-L137 EVAL"/>
<attribute name="OC_FARNELL" value="1831923"/>
<attribute name="OC_NEWARK" value="78R2891"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320C64X_DSP" prefix="IC">
<description>&lt;b&gt;TMS320C64x+ digital signal processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus-webapps.ti.com .. sprm148b.bsd&lt;br&gt;
&lt;i&gt;Connect-List generated from &lt;/i&gt;&lt;b&gt;TMS320C64X_DSP.DEV&lt;/b&gt; Variant &lt;b&gt;''&lt;/b&gt; with &lt;i&gt;&lt;b&gt;connect-device-split-symbol-03.ulp&lt;/b&gt;&lt;/i&gt;</description>
<gates>
<gate name="A" symbol="TMS320C64X_DSP-A"/>
<gate name="B" symbol="TMS320C64X_DSP-B"/>
<gate name="C" symbol="TMS320C64X_DSP-C"/>
<gate name="P" symbol="TMS320C64X_DSP-P"/>
</gates>
<devices>
<device name="" package="GTS_S-PBGA-N288">
<connects>
<connect gate="A" pin="AARDY" pad="L21"/>
<connect gate="A" pin="ABE_Z3" pad="AB21"/>
<connect gate="A" pin="ABE_Z4" pad="P21"/>
<connect gate="A" pin="ABE_Z5" pad="A22"/>
<connect gate="A" pin="ABE_Z6" pad="D16"/>
<connect gate="A" pin="ABUSREQ" pad="R19"/>
<connect gate="A" pin="ACE_Z3" pad="H19"/>
<connect gate="A" pin="ACE_Z4" pad="N20"/>
<connect gate="A" pin="ACE_Z5" pad="R20"/>
<connect gate="A" pin="ACE_Z6" pad="F20"/>
<connect gate="A" pin="ACLKR0" pad="K1"/>
<connect gate="A" pin="ACLKX0" pad="M1"/>
<connect gate="A" pin="AEA22" pad="M21"/>
<connect gate="A" pin="AEA23" pad="N21"/>
<connect gate="A" pin="AEA24" pad="P22"/>
<connect gate="A" pin="AEA25" pad="N22"/>
<connect gate="A" pin="AEA26" pad="H22"/>
<connect gate="A" pin="AEA27" pad="H21"/>
<connect gate="A" pin="AEA28" pad="J20"/>
<connect gate="A" pin="AEA29" pad="H20"/>
<connect gate="A" pin="AEA30" pad="G20"/>
<connect gate="A" pin="AEA31" pad="K20"/>
<connect gate="A" pin="AEA32" pad="B21"/>
<connect gate="A" pin="AEA33" pad="B22"/>
<connect gate="A" pin="AEA34" pad="D21"/>
<connect gate="A" pin="AEA35" pad="D22"/>
<connect gate="A" pin="AEA36" pad="E21"/>
<connect gate="A" pin="AEA37" pad="E22"/>
<connect gate="A" pin="AEA38" pad="F21"/>
<connect gate="A" pin="AEA39" pad="M20"/>
<connect gate="A" pin="AEA40" pad="J19"/>
<connect gate="A" pin="AEA41" pad="L20"/>
<connect gate="A" pin="AECLKIN" pad="K22"/>
<connect gate="A" pin="AECLKOUT1" pad="F22"/>
<connect gate="A" pin="AECLKOUT2" pad="U22"/>
<connect gate="A" pin="AED31" pad="W21"/>
<connect gate="A" pin="AED32" pad="W22"/>
<connect gate="A" pin="AED33" pad="V20"/>
<connect gate="A" pin="AED34" pad="W20"/>
<connect gate="A" pin="AED35" pad="AA22"/>
<connect gate="A" pin="AED36" pad="Y20"/>
<connect gate="A" pin="AED37" pad="AA21"/>
<connect gate="A" pin="AED38" pad="AB22"/>
<connect gate="A" pin="AED39" pad="P20"/>
<connect gate="A" pin="AED40" pad="R22"/>
<connect gate="A" pin="AED41" pad="R21"/>
<connect gate="A" pin="AED42" pad="U21"/>
<connect gate="A" pin="AED43" pad="V21"/>
<connect gate="A" pin="AED44" pad="T20"/>
<connect gate="A" pin="AED45" pad="V22"/>
<connect gate="A" pin="AED46" pad="U20"/>
<connect gate="A" pin="AED47" pad="A18"/>
<connect gate="A" pin="AED48" pad="D17"/>
<connect gate="A" pin="AED49" pad="B18"/>
<connect gate="A" pin="AED50" pad="C18"/>
<connect gate="A" pin="AED51" pad="A19"/>
<connect gate="A" pin="AED52" pad="C19"/>
<connect gate="A" pin="AED53" pad="B19"/>
<connect gate="A" pin="AED54" pad="A21"/>
<connect gate="A" pin="AED55" pad="D15"/>
<connect gate="A" pin="AED56" pad="A15"/>
<connect gate="A" pin="AED57" pad="B15"/>
<connect gate="A" pin="AED58" pad="C15"/>
<connect gate="A" pin="AED59" pad="A16"/>
<connect gate="A" pin="AED60" pad="C16"/>
<connect gate="A" pin="AED61" pad="B16"/>
<connect gate="A" pin="AED62" pad="C17"/>
<connect gate="A" pin="AFSR0" pad="K2"/>
<connect gate="A" pin="AFSX0" pad="M2"/>
<connect gate="A" pin="AHCLKR0" pad="L1"/>
<connect gate="A" pin="AHCLKX0" pad="N1"/>
<connect gate="A" pin="AHOLDA_Z" pad="J21"/>
<connect gate="A" pin="AHOLD_Z" pad="J22"/>
<connect gate="A" pin="AMUTE0" pad="K4"/>
<connect gate="A" pin="AMUTEIN0" pad="J4"/>
<connect gate="A" pin="APDTD_Z" pad="T19"/>
<connect gate="A" pin="ASDCAS_Z" pad="D20"/>
<connect gate="A" pin="ASDCKE" pad="K21"/>
<connect gate="A" pin="ASDRAS_Z" pad="E20"/>
<connect gate="A" pin="ASDWE_Z" pad="C20"/>
<connect gate="A" pin="ASOE3_Z" pad="P19"/>
<connect gate="A" pin="AXR010" pad="L2"/>
<connect gate="A" pin="AXR05" pad="P3"/>
<connect gate="A" pin="AXR06" pad="N3"/>
<connect gate="A" pin="AXR07" pad="M3"/>
<connect gate="A" pin="AXR08" pad="L3"/>
<connect gate="A" pin="AXR09" pad="K3"/>
<connect gate="B" pin="CLKIN" pad="A12"/>
<connect gate="B" pin="CLKINSEL" pad="A11"/>
<connect gate="B" pin="CLKMODE3" pad="C11"/>
<connect gate="B" pin="CLKMODE4" pad="B10"/>
<connect gate="B" pin="CLKMODE5" pad="A13"/>
<connect gate="B" pin="CLKMODE6" pad="C13"/>
<connect gate="B" pin="CLKOUT4" pad="A2"/>
<connect gate="B" pin="CLKOUT6" pad="B3"/>
<connect gate="B" pin="CLKR0" pad="C2"/>
<connect gate="B" pin="CLKR1" pad="G3"/>
<connect gate="B" pin="CLKS0" pad="D3"/>
<connect gate="B" pin="CLKS1" pad="G1"/>
<connect gate="B" pin="CLKX0" pad="E3"/>
<connect gate="B" pin="CLKX1" pad="H1"/>
<connect gate="B" pin="DR0" pad="D2"/>
<connect gate="B" pin="DR1" pad="F1"/>
<connect gate="B" pin="DX0" pad="E2"/>
<connect gate="B" pin="DX1" pad="H2"/>
<connect gate="B" pin="EMU0" pad="R1"/>
<connect gate="B" pin="EMU1" pad="T3"/>
<connect gate="B" pin="EMU10" pad="W3"/>
<connect gate="B" pin="EMU11" pad="W2"/>
<connect gate="B" pin="EMU2" pad="R2"/>
<connect gate="B" pin="EMU3" pad="U2"/>
<connect gate="B" pin="EMU4" pad="R3"/>
<connect gate="B" pin="EMU5" pad="P2"/>
<connect gate="B" pin="EMU6" pad="R4"/>
<connect gate="B" pin="EMU7" pad="V2"/>
<connect gate="B" pin="EMU8" pad="V1"/>
<connect gate="B" pin="EMU9" pad="V3"/>
<connect gate="B" pin="EXT_INT4_Z" pad="A4"/>
<connect gate="B" pin="EXT_INT5_Z" pad="B4"/>
<connect gate="B" pin="EXT_INT6_Z" pad="C4"/>
<connect gate="B" pin="EXT_INT7_Z" pad="Y1"/>
<connect gate="B" pin="RSV01" pad="B11"/>
<connect gate="B" pin="RSV02" pad="B12"/>
<connect gate="B" pin="RSV03" pad="D7"/>
<connect gate="B" pin="RSV04" pad="D8"/>
<connect gate="B" pin="RSV05" pad="C10"/>
<connect gate="B" pin="RSV06" pad="C8"/>
<connect gate="B" pin="RSV07" pad="U4"/>
<connect gate="B" pin="RSV08" pad="F3"/>
<connect gate="C" pin="FSR0" pad="D1"/>
<connect gate="C" pin="FSR1" pad="G2"/>
<connect gate="C" pin="FSX0" pad="E4"/>
<connect gate="C" pin="FSX1" pad="H3"/>
<connect gate="C" pin="GP0_00" pad="D13"/>
<connect gate="C" pin="GP0_03" pad="B13"/>
<connect gate="C" pin="HAS_Z" pad="Y5"/>
<connect gate="C" pin="HCNTL1" pad="W7"/>
<connect gate="C" pin="HCNTL2" pad="Y6"/>
<connect gate="C" pin="HCS_Z" pad="AA11"/>
<connect gate="C" pin="HD31" pad="Y8"/>
<connect gate="C" pin="HD32" pad="Y11"/>
<connect gate="C" pin="HD33" pad="W11"/>
<connect gate="C" pin="HD34" pad="W10"/>
<connect gate="C" pin="HD35" pad="Y4"/>
<connect gate="C" pin="HD36" pad="AB4"/>
<connect gate="C" pin="HD37" pad="AA9"/>
<connect gate="C" pin="HD38" pad="AA4"/>
<connect gate="C" pin="HD39" pad="AB9"/>
<connect gate="C" pin="HD40" pad="AB5"/>
<connect gate="C" pin="HD41" pad="Y9"/>
<connect gate="C" pin="HD42" pad="AB8"/>
<connect gate="C" pin="HD43" pad="AA6"/>
<connect gate="C" pin="HD44" pad="AB7"/>
<connect gate="C" pin="HD45" pad="AA7"/>
<connect gate="C" pin="HD46" pad="AB6"/>
<connect gate="C" pin="HD47" pad="Y12"/>
<connect gate="C" pin="HD48" pad="AA12"/>
<connect gate="C" pin="HD49" pad="AB13"/>
<connect gate="C" pin="HD50" pad="Y14"/>
<connect gate="C" pin="HD51" pad="AB14"/>
<connect gate="C" pin="HD52" pad="AA15"/>
<connect gate="C" pin="HD53" pad="Y16"/>
<connect gate="C" pin="HD54" pad="AB16"/>
<connect gate="C" pin="HD55" pad="W12"/>
<connect gate="C" pin="HD56" pad="AA13"/>
<connect gate="C" pin="HD57" pad="Y13"/>
<connect gate="C" pin="HD58" pad="AA14"/>
<connect gate="C" pin="HD59" pad="AB15"/>
<connect gate="C" pin="HD60" pad="AA16"/>
<connect gate="C" pin="HD61" pad="Y15"/>
<connect gate="C" pin="HD62" pad="W15"/>
<connect gate="C" pin="HDS1_Z" pad="AB11"/>
<connect gate="C" pin="HDS2_Z" pad="AB12"/>
<connect gate="C" pin="HHWIL" pad="Y7"/>
<connect gate="C" pin="HINT_Z" pad="AA8"/>
<connect gate="C" pin="HRDY_Z" pad="Y10"/>
<connect gate="C" pin="HRW" pad="AA5"/>
<connect gate="C" pin="NMI" pad="B9"/>
<connect gate="C" pin="OSCIN" pad="A6"/>
<connect gate="C" pin="OSCOUT" pad="A7"/>
<connect gate="C" pin="OSCVDD" pad="B6"/>
<connect gate="C" pin="OSCVSS" pad="C6"/>
<connect gate="C" pin="OSC_DIS" pad="B7"/>
<connect gate="C" pin="PLLV" pad="C12"/>
<connect gate="C" pin="RESET_Z" pad="C9"/>
<connect gate="C" pin="SCL0" pad="AB18"/>
<connect gate="C" pin="SCL1" pad="AA18"/>
<connect gate="C" pin="SDA0" pad="AB19"/>
<connect gate="C" pin="SDA1" pad="AA19"/>
<connect gate="C" pin="TCK" pad="T2"/>
<connect gate="C" pin="TDI" pad="T1"/>
<connect gate="C" pin="TDO" pad="T4"/>
<connect gate="C" pin="TINP0" pad="AB2"/>
<connect gate="C" pin="TINP1" pad="AB1"/>
<connect gate="C" pin="TMS" pad="U3"/>
<connect gate="C" pin="TOUT0" pad="AA2"/>
<connect gate="C" pin="TOUT1" pad="AA1"/>
<connect gate="C" pin="TRST_Z" pad="U1"/>
<connect gate="P" pin="CVDD@21" pad="D5"/>
<connect gate="P" pin="CVDD@22" pad="D6"/>
<connect gate="P" pin="CVDD@23" pad="D9"/>
<connect gate="P" pin="CVDD@24" pad="D11"/>
<connect gate="P" pin="CVDD@25" pad="D12"/>
<connect gate="P" pin="CVDD@26" pad="D14"/>
<connect gate="P" pin="CVDD@27" pad="D18"/>
<connect gate="P" pin="CVDD@28" pad="E19"/>
<connect gate="P" pin="CVDD@29" pad="F19"/>
<connect gate="P" pin="CVDD@30" pad="G4"/>
<connect gate="P" pin="CVDD@31" pad="H4"/>
<connect gate="P" pin="CVDD@32" pad="L19"/>
<connect gate="P" pin="CVDD@33" pad="M4"/>
<connect gate="P" pin="CVDD@34" pad="M19"/>
<connect gate="P" pin="CVDD@35" pad="N4"/>
<connect gate="P" pin="CVDD@36" pad="V4"/>
<connect gate="P" pin="CVDD@37" pad="V19"/>
<connect gate="P" pin="CVDD@38" pad="W5"/>
<connect gate="P" pin="CVDD@39" pad="W9"/>
<connect gate="P" pin="CVDD@40" pad="W13"/>
<connect gate="P" pin="CVDD@41" pad="W16"/>
<connect gate="P" pin="CVDD@42" pad="W18"/>
<connect gate="P" pin="DVDD@23" pad="A3"/>
<connect gate="P" pin="DVDD@24" pad="A5"/>
<connect gate="P" pin="DVDD@25" pad="A8"/>
<connect gate="P" pin="DVDD@26" pad="A9"/>
<connect gate="P" pin="DVDD@27" pad="A14"/>
<connect gate="P" pin="DVDD@28" pad="A17"/>
<connect gate="P" pin="DVDD@29" pad="A20"/>
<connect gate="P" pin="DVDD@30" pad="B1"/>
<connect gate="P" pin="DVDD@31" pad="C22"/>
<connect gate="P" pin="DVDD@32" pad="E1"/>
<connect gate="P" pin="DVDD@33" pad="G22"/>
<connect gate="P" pin="DVDD@34" pad="J1"/>
<connect gate="P" pin="DVDD@35" pad="M22"/>
<connect gate="P" pin="DVDD@36" pad="P1"/>
<connect gate="P" pin="DVDD@37" pad="T22"/>
<connect gate="P" pin="DVDD@38" pad="W1"/>
<connect gate="P" pin="DVDD@39" pad="Y2"/>
<connect gate="P" pin="DVDD@40" pad="Y17"/>
<connect gate="P" pin="DVDD@41" pad="Y19"/>
<connect gate="P" pin="DVDD@42" pad="Y22"/>
<connect gate="P" pin="DVDD@43" pad="AB3"/>
<connect gate="P" pin="DVDD@44" pad="AB10"/>
<connect gate="P" pin="DVDD@45" pad="AB17"/>
<connect gate="P" pin="DVDD@46" pad="AB20"/>
<connect gate="P" pin="VSS@43" pad="A1"/>
<connect gate="P" pin="VSS@44" pad="A10"/>
<connect gate="P" pin="VSS@45" pad="B2"/>
<connect gate="P" pin="VSS@46" pad="B5"/>
<connect gate="P" pin="VSS@47" pad="B8"/>
<connect gate="P" pin="VSS@48" pad="B14"/>
<connect gate="P" pin="VSS@49" pad="B17"/>
<connect gate="P" pin="VSS@50" pad="B20"/>
<connect gate="P" pin="VSS@51" pad="C1"/>
<connect gate="P" pin="VSS@52" pad="C3"/>
<connect gate="P" pin="VSS@53" pad="C5"/>
<connect gate="P" pin="VSS@54" pad="C7"/>
<connect gate="P" pin="VSS@55" pad="C14"/>
<connect gate="P" pin="VSS@56" pad="C21"/>
<connect gate="P" pin="VSS@57" pad="D4"/>
<connect gate="P" pin="VSS@58" pad="D10"/>
<connect gate="P" pin="VSS@59" pad="D19"/>
<connect gate="P" pin="VSS@60" pad="F2"/>
<connect gate="P" pin="VSS@61" pad="F4"/>
<connect gate="P" pin="VSS@62" pad="G19"/>
<connect gate="P" pin="VSS@63" pad="G21"/>
<connect gate="P" pin="VSS@64" pad="J2"/>
<connect gate="P" pin="VSS@65" pad="J3"/>
<connect gate="P" pin="VSS@66" pad="K19"/>
<connect gate="P" pin="VSS@67" pad="L4"/>
<connect gate="P" pin="VSS@68" pad="L22"/>
<connect gate="P" pin="VSS@69" pad="N2"/>
<connect gate="P" pin="VSS@70" pad="N19"/>
<connect gate="P" pin="VSS@71" pad="P4"/>
<connect gate="P" pin="VSS@72" pad="T21"/>
<connect gate="P" pin="VSS@73" pad="U19"/>
<connect gate="P" pin="VSS@74" pad="W4"/>
<connect gate="P" pin="VSS@75" pad="W6"/>
<connect gate="P" pin="VSS@76" pad="W8"/>
<connect gate="P" pin="VSS@77" pad="W14"/>
<connect gate="P" pin="VSS@78" pad="W17"/>
<connect gate="P" pin="VSS@79" pad="W19"/>
<connect gate="P" pin="VSS@80" pad="Y3"/>
<connect gate="P" pin="VSS@81" pad="Y18"/>
<connect gate="P" pin="VSS@82" pad="Y21"/>
<connect gate="P" pin="VSS@83" pad="AA3"/>
<connect gate="P" pin="VSS@84" pad="AA10"/>
<connect gate="P" pin="VSS@85" pad="AA17"/>
<connect gate="P" pin="VSS@86" pad="AA20"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1610186"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320C6474" prefix="IC">
<description>&lt;b&gt;TMS320C6474 Multicore Digital Signal Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: sprm335.bsd&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/tms320c6474.pdf&lt;br&gt;&lt;i&gt;Connect-List generated from &lt;/i&gt;&lt;b&gt;TMS320C6474.DEV&lt;/b&gt; Variant &lt;b&gt;''&lt;/b&gt; with &lt;i&gt;&lt;b&gt;connect-device-split-symbol-03.ulp&lt;/b&gt;&lt;/i&gt;</description>
<gates>
<gate name="A" symbol="TMS320C6474-A"/>
<gate name="B" symbol="TMS320C6474-B"/>
<gate name="C" symbol="TMS320C6474-C"/>
<gate name="D" symbol="TMS320C6474-D"/>
<gate name="P" symbol="TMS320C6474-P"/>
</gates>
<devices>
<device name="" package="ZUN_SPBGA-N561">
<connects>
<connect gate="A" pin="AIFRXN0" pad="AF22"/>
<connect gate="A" pin="AIFRXN1" pad="AG20"/>
<connect gate="A" pin="AIFRXN2" pad="AG18"/>
<connect gate="A" pin="AIFRXN3" pad="AE17"/>
<connect gate="A" pin="AIFRXN4" pad="AE14"/>
<connect gate="A" pin="AIFRXN5" pad="AF12"/>
<connect gate="A" pin="AIFRXP0" pad="AF21"/>
<connect gate="A" pin="AIFRXP1" pad="AG21"/>
<connect gate="A" pin="AIFRXP2" pad="AG17"/>
<connect gate="A" pin="AIFRXP3" pad="AE18"/>
<connect gate="A" pin="AIFRXP4" pad="AE13"/>
<connect gate="A" pin="AIFRXP5" pad="AF13"/>
<connect gate="A" pin="AIFTXN0" pad="AE21"/>
<connect gate="A" pin="AIFTXN1" pad="AD21"/>
<connect gate="A" pin="AIFTXN2" pad="AF16"/>
<connect gate="A" pin="AIFTXN3" pad="AD17"/>
<connect gate="A" pin="AIFTXN4" pad="AG13"/>
<connect gate="A" pin="AIFTXN5" pad="AD13"/>
<connect gate="A" pin="AIFTXP0" pad="AE22"/>
<connect gate="A" pin="AIFTXP1" pad="AD20"/>
<connect gate="A" pin="AIFTXP2" pad="AF17"/>
<connect gate="A" pin="AIFTXP3" pad="AD16"/>
<connect gate="A" pin="AIFTXP4" pad="AG14"/>
<connect gate="A" pin="AIFTXP5" pad="AD12"/>
<connect gate="A" pin="ALTCORECLKN" pad="AF10"/>
<connect gate="A" pin="ALTCORECLKP" pad="AF9"/>
<connect gate="A" pin="ALTFSYNCCLK" pad="AF6"/>
<connect gate="A" pin="ALTFSYNCPULSE" pad="AE6"/>
<connect gate="B" pin="CLKR0" pad="B20"/>
<connect gate="B" pin="CLKR1" pad="A24"/>
<connect gate="B" pin="CLKS0" pad="D20"/>
<connect gate="B" pin="CLKS1" pad="A25"/>
<connect gate="B" pin="CLKX0" pad="C20"/>
<connect gate="B" pin="CLKX1" pad="C22"/>
<connect gate="B" pin="CORECLKSEL" pad="AF7"/>
<connect gate="B" pin="DDRA00" pad="K25"/>
<connect gate="B" pin="DDRA01" pad="N25"/>
<connect gate="B" pin="DDRA02" pad="M25"/>
<connect gate="B" pin="DDRA03" pad="R26"/>
<connect gate="B" pin="DDRA04" pad="L25"/>
<connect gate="B" pin="DDRA05" pad="N27"/>
<connect gate="B" pin="DDRA06" pad="L26"/>
<connect gate="B" pin="DDRA07" pad="U26"/>
<connect gate="B" pin="DDRA08" pad="K26"/>
<connect gate="B" pin="DDRA09" pad="R27"/>
<connect gate="B" pin="DDRA10" pad="P25"/>
<connect gate="B" pin="DDRA11" pad="L27"/>
<connect gate="B" pin="DDRA12" pad="U27"/>
<connect gate="B" pin="DDRA13" pad="K27"/>
<connect gate="B" pin="DDRBA0" pad="T25"/>
<connect gate="B" pin="DDRBA1" pad="R25"/>
<connect gate="B" pin="DDRBA2" pad="U25"/>
<connect gate="B" pin="DDRCASZ" pad="N26"/>
<connect gate="B" pin="DDRCEZ" pad="L24"/>
<connect gate="B" pin="DDRCKE" pad="T24"/>
<connect gate="B" pin="DDRCLKOUTN0" pad="V24"/>
<connect gate="B" pin="DDRCLKOUTN1" pad="J24"/>
<connect gate="B" pin="DDRCLKOUTP0" pad="V25"/>
<connect gate="B" pin="DDRCLKOUTP1" pad="J25"/>
<connect gate="B" pin="DDRD00" pad="W27"/>
<connect gate="B" pin="DDRD01" pad="W25"/>
<connect gate="B" pin="DDRD02" pad="Y27"/>
<connect gate="B" pin="DDRD03" pad="W26"/>
<connect gate="B" pin="DDRD04" pad="AA27"/>
<connect gate="B" pin="DDRD05" pad="AA26"/>
<connect gate="B" pin="DDRD06" pad="AA25"/>
<connect gate="B" pin="DDRD07" pad="AA24"/>
<connect gate="B" pin="DDRD08" pad="AC27"/>
<connect gate="B" pin="DDRD09" pad="AC26"/>
<connect gate="B" pin="DDRD10" pad="AC25"/>
<connect gate="B" pin="DDRD11" pad="AD27"/>
<connect gate="B" pin="DDRD12" pad="AC24"/>
<connect gate="B" pin="DDRD13" pad="AE26"/>
<connect gate="B" pin="DDRD14" pad="AE27"/>
<connect gate="B" pin="DDRD15" pad="AE25"/>
<connect gate="B" pin="DDRD16" pad="B25"/>
<connect gate="B" pin="DDRD17" pad="D25"/>
<connect gate="B" pin="DDRD18" pad="B26"/>
<connect gate="B" pin="DDRD19" pad="D24"/>
<connect gate="B" pin="DDRD20" pad="B27"/>
<connect gate="B" pin="DDRD21" pad="D26"/>
<connect gate="B" pin="DDRD22" pad="D27"/>
<connect gate="B" pin="DDRD23" pad="C27"/>
<connect gate="B" pin="DDRD24" pad="F24"/>
<connect gate="B" pin="DDRD25" pad="F25"/>
<connect gate="B" pin="DDRD26" pad="F26"/>
<connect gate="B" pin="DDRD27" pad="F27"/>
<connect gate="B" pin="DDRD28" pad="G27"/>
<connect gate="B" pin="DDRD29" pad="H25"/>
<connect gate="B" pin="DDRD30" pad="H26"/>
<connect gate="B" pin="DDRD31" pad="H27"/>
<connect gate="B" pin="DDRDQM0" pad="W24"/>
<connect gate="B" pin="DDRDQM1" pad="AE24"/>
<connect gate="B" pin="DDRDQM2" pad="B24"/>
<connect gate="B" pin="DDRDQM3" pad="H24"/>
<connect gate="B" pin="DDRDQS0N" pad="Y25"/>
<connect gate="B" pin="DDRDQS0P" pad="Y26"/>
<connect gate="B" pin="DDRDQS1N" pad="AD25"/>
<connect gate="B" pin="DDRDQS1P" pad="AD26"/>
<connect gate="B" pin="DDRDQS2N" pad="C25"/>
<connect gate="B" pin="DDRDQS2P" pad="C26"/>
<connect gate="B" pin="DDRDQS3N" pad="G26"/>
<connect gate="B" pin="DDRDQS3P" pad="G25"/>
<connect gate="B" pin="DDRODT" pad="K24"/>
<connect gate="B" pin="DDRRASZ" pad="M24"/>
<connect gate="B" pin="DDRRCVENIN0" pad="AB25"/>
<connect gate="B" pin="DDRRCVENIN1" pad="E24"/>
<connect gate="B" pin="DDRRCVENOUT0" pad="AB24"/>
<connect gate="B" pin="DDRRCVENOUT1" pad="E25"/>
<connect gate="B" pin="DDRREFCLKN" pad="AD23"/>
<connect gate="B" pin="DDRREFCLKP" pad="AD24"/>
<connect gate="B" pin="DDRSLRATE" pad="AE23"/>
<connect gate="B" pin="DDRWEZ" pad="P24"/>
<connect gate="B" pin="DR0" pad="A20"/>
<connect gate="B" pin="DR1" pad="D21"/>
<connect gate="B" pin="DX0" pad="D19"/>
<connect gate="B" pin="DX1" pad="B22"/>
<connect gate="C" pin="EMU00" pad="R4"/>
<connect gate="C" pin="EMU01" pad="R2"/>
<connect gate="C" pin="EMU02" pad="N3"/>
<connect gate="C" pin="EMU03" pad="N1"/>
<connect gate="C" pin="EMU04" pad="M2"/>
<connect gate="C" pin="EMU05" pad="M1"/>
<connect gate="C" pin="EMU06" pad="N4"/>
<connect gate="C" pin="EMU07" pad="R3"/>
<connect gate="C" pin="EMU08" pad="M4"/>
<connect gate="C" pin="EMU09" pad="N2"/>
<connect gate="C" pin="EMU10" pad="R1"/>
<connect gate="C" pin="EMU11" pad="T2"/>
<connect gate="C" pin="EMU12" pad="L3"/>
<connect gate="C" pin="EMU13" pad="P4"/>
<connect gate="C" pin="EMU14" pad="K2"/>
<connect gate="C" pin="EMU15" pad="T1"/>
<connect gate="C" pin="EMU16" pad="P3"/>
<connect gate="C" pin="EMU17" pad="L4"/>
<connect gate="C" pin="EMU18" pad="M3"/>
<connect gate="C" pin="FRAMEBURSTN" pad="AD10"/>
<connect gate="C" pin="FRAMEBURSTP" pad="AD9"/>
<connect gate="C" pin="FSR0" pad="B21"/>
<connect gate="C" pin="FSR1" pad="C21"/>
<connect gate="C" pin="FSX0" pad="A21"/>
<connect gate="C" pin="FSX1" pad="A22"/>
<connect gate="C" pin="FSYNCCLKN" pad="AD8"/>
<connect gate="C" pin="FSYNCCLKP" pad="AD7"/>
<connect gate="C" pin="GP00" pad="T3"/>
<connect gate="C" pin="GP01" pad="U4"/>
<connect gate="C" pin="GP02" pad="V1"/>
<connect gate="C" pin="GP03" pad="U3"/>
<connect gate="C" pin="GP04" pad="T4"/>
<connect gate="C" pin="GP05" pad="V2"/>
<connect gate="C" pin="GP06" pad="V3"/>
<connect gate="C" pin="GP07" pad="Y3"/>
<connect gate="C" pin="GP08" pad="Y4"/>
<connect gate="C" pin="GP09" pad="AA2"/>
<connect gate="C" pin="GP10" pad="AA3"/>
<connect gate="C" pin="GP11" pad="AB4"/>
<connect gate="C" pin="GP12" pad="AB3"/>
<connect gate="C" pin="GP13" pad="AB2"/>
<connect gate="C" pin="GP14" pad="AA4"/>
<connect gate="C" pin="GP15" pad="AC3"/>
<connect gate="C" pin="MDCLK" pad="C19"/>
<connect gate="C" pin="MDIO" pad="B19"/>
<connect gate="C" pin="NMI0" pad="J4"/>
<connect gate="C" pin="NMI1" pad="J2"/>
<connect gate="C" pin="NMI2" pad="J1"/>
<connect gate="D" pin="PORZ" pad="AE5"/>
<connect gate="D" pin="RESETSTATZ" pad="AF4"/>
<connect gate="D" pin="RIORXN0" pad="A9"/>
<connect gate="D" pin="RIORXN1" pad="A13"/>
<connect gate="D" pin="RIORXP0" pad="A10"/>
<connect gate="D" pin="RIORXP1" pad="A12"/>
<connect gate="D" pin="RIOSGMIICLKN" pad="D9"/>
<connect gate="D" pin="RIOSGMIICLKP" pad="C9"/>
<connect gate="D" pin="RIOTXN0" pad="C11"/>
<connect gate="D" pin="RIOTXN1" pad="C13"/>
<connect gate="D" pin="RIOTXP0" pad="C10"/>
<connect gate="D" pin="RIOTXP1" pad="C14"/>
<connect gate="D" pin="RSV01" pad="AE19"/>
<connect gate="D" pin="RSV02" pad="AD14"/>
<connect gate="D" pin="RSV03" pad="N24"/>
<connect gate="D" pin="RSV04" pad="AG10"/>
<connect gate="D" pin="RSV05" pad="AG24"/>
<connect gate="D" pin="RSV06" pad="AE7"/>
<connect gate="D" pin="RSV07" pad="AE8"/>
<connect gate="D" pin="RSV08" pad="AF24"/>
<connect gate="D" pin="RSV09" pad="AF25"/>
<connect gate="D" pin="RSV10" pad="K4"/>
<connect gate="D" pin="RSV11" pad="K3"/>
<connect gate="D" pin="RSV12" pad="K1"/>
<connect gate="D" pin="RSV13" pad="G4"/>
<connect gate="D" pin="RSV14" pad="F3"/>
<connect gate="D" pin="RSV15" pad="D7"/>
<connect gate="D" pin="RSV16" pad="C7"/>
<connect gate="D" pin="RSV17" pad="B12"/>
<connect gate="D" pin="RSV18" pad="B18"/>
<connect gate="D" pin="RSV19" pad="D6"/>
<connect gate="D" pin="RSV20" pad="C6"/>
<connect gate="D" pin="RSV21" pad="E6"/>
<connect gate="D" pin="RSV22" pad="E7"/>
<connect gate="D" pin="RSV23" pad="AE4"/>
<connect gate="D" pin="RSV24" pad="AG25"/>
<connect gate="D" pin="RSV25" pad="D22"/>
<connect gate="D" pin="RSV26" pad="C23"/>
<connect gate="D" pin="RSV27" pad="D5"/>
<connect gate="D" pin="RSV28" pad="C5"/>
<connect gate="D" pin="RSV29" pad="J3"/>
<connect gate="D" pin="SCL" pad="E4"/>
<connect gate="D" pin="SDA" pad="D4"/>
<connect gate="D" pin="SGMIIRXN" pad="C16"/>
<connect gate="D" pin="SGMIIRXP" pad="C17"/>
<connect gate="D" pin="SGMIITXN" pad="A16"/>
<connect gate="D" pin="SGMIITXP" pad="A15"/>
<connect gate="D" pin="SMFRAMECLK" pad="AD4"/>
<connect gate="D" pin="SYSCLKN" pad="AE10"/>
<connect gate="D" pin="SYSCLKOUT" pad="AD6"/>
<connect gate="D" pin="SYSCLKP" pad="AE9"/>
<connect gate="D" pin="TCK" pad="W4"/>
<connect gate="D" pin="TDI" pad="V4"/>
<connect gate="D" pin="TDO" pad="W3"/>
<connect gate="D" pin="TIMI0" pad="E3"/>
<connect gate="D" pin="TIMI1" pad="C4"/>
<connect gate="D" pin="TIMO0" pad="F2"/>
<connect gate="D" pin="TIMO1" pad="F4"/>
<connect gate="D" pin="TMS" pad="W1"/>
<connect gate="D" pin="TRSTZ" pad="W2"/>
<connect gate="D" pin="TRT" pad="AD3"/>
<connect gate="D" pin="TRTCLK" pad="AC4"/>
<connect gate="D" pin="VCNTL0" pad="G3"/>
<connect gate="D" pin="VCNTL1" pad="G2"/>
<connect gate="D" pin="VCNTL2" pad="H4"/>
<connect gate="D" pin="VCNTL3" pad="H3"/>
<connect gate="D" pin="VREFSSTL" pad="T26"/>
<connect gate="P" pin="AIF_VDDA_11" pad="AC12"/>
<connect gate="P" pin="AIF_VDDA_11@1" pad="AC15"/>
<connect gate="P" pin="AIF_VDDA_11@10" pad="W19"/>
<connect gate="P" pin="AIF_VDDA_11@2" pad="AC18"/>
<connect gate="P" pin="AIF_VDDA_11@3" pad="AC21"/>
<connect gate="P" pin="AIF_VDDA_11@4" pad="AG26"/>
<connect gate="P" pin="AIF_VDDA_11@5" pad="U17"/>
<connect gate="P" pin="AIF_VDDA_11@6" pad="V16"/>
<connect gate="P" pin="AIF_VDDA_11@7" pad="V18"/>
<connect gate="P" pin="AIF_VDDA_11@8" pad="W15"/>
<connect gate="P" pin="AIF_VDDA_11@9" pad="W17"/>
<connect gate="P" pin="AIF_VDDR_18" pad="AD19"/>
<connect gate="P" pin="AIF_VDDR_18@1" pad="AD15"/>
<connect gate="P" pin="AIF_VDDT_11" pad="AC11"/>
<connect gate="P" pin="AIF_VDDT_11@1" pad="AC14"/>
<connect gate="P" pin="AIF_VDDT_11@2" pad="AC17"/>
<connect gate="P" pin="AIF_VDDT_11@3" pad="AC20"/>
<connect gate="P" pin="AIF_VDDT_11@4" pad="AF15"/>
<connect gate="P" pin="AIF_VDDT_11@5" pad="AF19"/>
<connect gate="P" pin="AIF_VDDT_11@6" pad="AG11"/>
<connect gate="P" pin="AVDD1_18" pad="AG9"/>
<connect gate="P" pin="AVDD2_18" pad="AG23"/>
<connect gate="P" pin="CVDD" pad="J11"/>
<connect gate="P" pin="CVDD@1" pad="J17"/>
<connect gate="P" pin="CVDD@10" pad="L19"/>
<connect gate="P" pin="CVDD@11" pad="L9"/>
<connect gate="P" pin="CVDD@12" pad="M10"/>
<connect gate="P" pin="CVDD@13" pad="M12"/>
<connect gate="P" pin="CVDD@14" pad="M14"/>
<connect gate="P" pin="CVDD@15" pad="M16"/>
<connect gate="P" pin="CVDD@16" pad="M18"/>
<connect gate="P" pin="CVDD@17" pad="N11"/>
<connect gate="P" pin="CVDD@18" pad="N13"/>
<connect gate="P" pin="CVDD@19" pad="N15"/>
<connect gate="P" pin="CVDD@2" pad="J19"/>
<connect gate="P" pin="CVDD@20" pad="N17"/>
<connect gate="P" pin="CVDD@21" pad="N19"/>
<connect gate="P" pin="CVDD@22" pad="N9"/>
<connect gate="P" pin="CVDD@23" pad="P10"/>
<connect gate="P" pin="CVDD@24" pad="P12"/>
<connect gate="P" pin="CVDD@25" pad="P14"/>
<connect gate="P" pin="CVDD@26" pad="P16"/>
<connect gate="P" pin="CVDD@27" pad="P18"/>
<connect gate="P" pin="CVDD@28" pad="R11"/>
<connect gate="P" pin="CVDD@29" pad="R13"/>
<connect gate="P" pin="CVDD@3" pad="J9"/>
<connect gate="P" pin="CVDD@30" pad="R15"/>
<connect gate="P" pin="CVDD@31" pad="R17"/>
<connect gate="P" pin="CVDD@32" pad="R19"/>
<connect gate="P" pin="CVDD@33" pad="R9"/>
<connect gate="P" pin="CVDD@34" pad="T10"/>
<connect gate="P" pin="CVDD@35" pad="T12"/>
<connect gate="P" pin="CVDD@36" pad="T14"/>
<connect gate="P" pin="CVDD@37" pad="T16"/>
<connect gate="P" pin="CVDD@38" pad="T18"/>
<connect gate="P" pin="CVDD@39" pad="U11"/>
<connect gate="P" pin="CVDD@4" pad="K10"/>
<connect gate="P" pin="CVDD@40" pad="U13"/>
<connect gate="P" pin="CVDD@41" pad="U15"/>
<connect gate="P" pin="CVDD@42" pad="U19"/>
<connect gate="P" pin="CVDD@43" pad="U9"/>
<connect gate="P" pin="CVDD@44" pad="V10"/>
<connect gate="P" pin="CVDD@45" pad="V12"/>
<connect gate="P" pin="CVDD@46" pad="V14"/>
<connect gate="P" pin="CVDD@47" pad="W11"/>
<connect gate="P" pin="CVDD@48" pad="W13"/>
<connect gate="P" pin="CVDD@49" pad="W9"/>
<connect gate="P" pin="CVDD@5" pad="K18"/>
<connect gate="P" pin="CVDD@6" pad="L11"/>
<connect gate="P" pin="CVDD@7" pad="L13"/>
<connect gate="P" pin="CVDD@8" pad="L15"/>
<connect gate="P" pin="CVDD@9" pad="L17"/>
<connect gate="P" pin="CVDD_MON" pad="AG6"/>
<connect gate="P" pin="DVDD_18" pad="A1"/>
<connect gate="P" pin="DVDD_18@1" pad="A19"/>
<connect gate="P" pin="DVDD_18@10" pad="AC5"/>
<connect gate="P" pin="DVDD_18@11" pad="AC7"/>
<connect gate="P" pin="DVDD_18@12" pad="AC9"/>
<connect gate="P" pin="DVDD_18@13" pad="AF5"/>
<connect gate="P" pin="DVDD_18@14" pad="AG1"/>
<connect gate="P" pin="DVDD_18@15" pad="AG27"/>
<connect gate="P" pin="DVDD_18@16" pad="AG8"/>
<connect gate="P" pin="DVDD_18@17" pad="E1"/>
<connect gate="P" pin="DVDD_18@18" pad="E19"/>
<connect gate="P" pin="DVDD_18@19" pad="E21"/>
<connect gate="P" pin="DVDD_18@2" pad="A23"/>
<connect gate="P" pin="DVDD_18@20" pad="E23"/>
<connect gate="P" pin="DVDD_18@21" pad="E27"/>
<connect gate="P" pin="DVDD_18@22" pad="E5"/>
<connect gate="P" pin="DVDD_18@23" pad="G23"/>
<connect gate="P" pin="DVDD_18@24" pad="G5"/>
<connect gate="P" pin="DVDD_18@25" pad="H2"/>
<connect gate="P" pin="DVDD_18@26" pad="J23"/>
<connect gate="P" pin="DVDD_18@27" pad="J27"/>
<connect gate="P" pin="DVDD_18@28" pad="J5"/>
<connect gate="P" pin="DVDD_18@29" pad="L1"/>
<connect gate="P" pin="DVDD_18@3" pad="A27"/>
<connect gate="P" pin="DVDD_18@30" pad="L23"/>
<connect gate="P" pin="DVDD_18@31" pad="L5"/>
<connect gate="P" pin="DVDD_18@32" pad="M26"/>
<connect gate="P" pin="DVDD_18@33" pad="N23"/>
<connect gate="P" pin="DVDD_18@34" pad="N5"/>
<connect gate="P" pin="DVDD_18@35" pad="P2"/>
<connect gate="P" pin="DVDD_18@36" pad="P26"/>
<connect gate="P" pin="DVDD_18@37" pad="R23"/>
<connect gate="P" pin="DVDD_18@38" pad="R5"/>
<connect gate="P" pin="DVDD_18@39" pad="U1"/>
<connect gate="P" pin="DVDD_18@4" pad="A5"/>
<connect gate="P" pin="DVDD_18@40" pad="U23"/>
<connect gate="P" pin="DVDD_18@41" pad="U5"/>
<connect gate="P" pin="DVDD_18@42" pad="V26"/>
<connect gate="P" pin="DVDD_18@43" pad="W23"/>
<connect gate="P" pin="DVDD_18@44" pad="W5"/>
<connect gate="P" pin="DVDD_18@45" pad="Y2"/>
<connect gate="P" pin="DVDD_18@46" pad="Y24"/>
<connect gate="P" pin="DVDD_18@5" pad="AA23"/>
<connect gate="P" pin="DVDD_18@6" pad="AA5"/>
<connect gate="P" pin="DVDD_18@7" pad="AB26"/>
<connect gate="P" pin="DVDD_18@8" pad="AC1"/>
<connect gate="P" pin="DVDD_18@9" pad="AC23"/>
<connect gate="P" pin="DVDD_18_MON" pad="AG7"/>
<connect gate="P" pin="SGR_VDDA_11" pad="D12"/>
<connect gate="P" pin="SGR_VDDA_11@1" pad="D18"/>
<connect gate="P" pin="SGR_VDDA_11@2" pad="E11"/>
<connect gate="P" pin="SGR_VDDA_11@3" pad="E15"/>
<connect gate="P" pin="SGR_VDDD_11" pad="J13"/>
<connect gate="P" pin="SGR_VDDD_11@1" pad="J15"/>
<connect gate="P" pin="SGR_VDDD_11@2" pad="K12"/>
<connect gate="P" pin="SGR_VDDD_11@3" pad="K14"/>
<connect gate="P" pin="SGR_VDDD_11@4" pad="K16"/>
<connect gate="P" pin="SGR_VDDR_18" pad="C12"/>
<connect gate="P" pin="SGR_VDDR_18@1" pad="A18"/>
<connect gate="P" pin="SGR_VDDT_11" pad="B13"/>
<connect gate="P" pin="SGR_VDDT_11@1" pad="B17"/>
<connect gate="P" pin="SGR_VDDT_11@2" pad="B8"/>
<connect gate="P" pin="SGR_VDDT_11@3" pad="E13"/>
<connect gate="P" pin="SGR_VDDT_11@4" pad="E17"/>
<connect gate="P" pin="SGR_VDDT_11@5" pad="E9"/>
<connect gate="P" pin="VSS" pad="A11"/>
<connect gate="P" pin="VSS@1" pad="A14"/>
<connect gate="P" pin="VSS@10" pad="AA1"/>
<connect gate="P" pin="VSS@100" pad="F23"/>
<connect gate="P" pin="VSS@101" pad="F5"/>
<connect gate="P" pin="VSS@102" pad="G1"/>
<connect gate="P" pin="VSS@103" pad="G24"/>
<connect gate="P" pin="VSS@104" pad="H1"/>
<connect gate="P" pin="VSS@105" pad="H23"/>
<connect gate="P" pin="VSS@106" pad="H5"/>
<connect gate="P" pin="VSS@107" pad="J10"/>
<connect gate="P" pin="VSS@108" pad="J12"/>
<connect gate="P" pin="VSS@109" pad="J14"/>
<connect gate="P" pin="VSS@11" pad="AB1"/>
<connect gate="P" pin="VSS@110" pad="J16"/>
<connect gate="P" pin="VSS@111" pad="J18"/>
<connect gate="P" pin="VSS@112" pad="J26"/>
<connect gate="P" pin="VSS@113" pad="K11"/>
<connect gate="P" pin="VSS@114" pad="K13"/>
<connect gate="P" pin="VSS@115" pad="K15"/>
<connect gate="P" pin="VSS@116" pad="K17"/>
<connect gate="P" pin="VSS@117" pad="K19"/>
<connect gate="P" pin="VSS@118" pad="K23"/>
<connect gate="P" pin="VSS@119" pad="K5"/>
<connect gate="P" pin="VSS@12" pad="AB23"/>
<connect gate="P" pin="VSS@120" pad="K9"/>
<connect gate="P" pin="VSS@121" pad="L10"/>
<connect gate="P" pin="VSS@122" pad="L12"/>
<connect gate="P" pin="VSS@123" pad="L14"/>
<connect gate="P" pin="VSS@124" pad="L16"/>
<connect gate="P" pin="VSS@125" pad="L18"/>
<connect gate="P" pin="VSS@126" pad="L2"/>
<connect gate="P" pin="VSS@127" pad="M11"/>
<connect gate="P" pin="VSS@128" pad="M13"/>
<connect gate="P" pin="VSS@129" pad="M15"/>
<connect gate="P" pin="VSS@13" pad="AB27"/>
<connect gate="P" pin="VSS@130" pad="M17"/>
<connect gate="P" pin="VSS@131" pad="M19"/>
<connect gate="P" pin="VSS@132" pad="M23"/>
<connect gate="P" pin="VSS@133" pad="M27"/>
<connect gate="P" pin="VSS@134" pad="M5"/>
<connect gate="P" pin="VSS@135" pad="M9"/>
<connect gate="P" pin="VSS@136" pad="N10"/>
<connect gate="P" pin="VSS@137" pad="N12"/>
<connect gate="P" pin="VSS@138" pad="N14"/>
<connect gate="P" pin="VSS@139" pad="N16"/>
<connect gate="P" pin="VSS@14" pad="AB5"/>
<connect gate="P" pin="VSS@140" pad="N18"/>
<connect gate="P" pin="VSS@141" pad="P1"/>
<connect gate="P" pin="VSS@142" pad="P11"/>
<connect gate="P" pin="VSS@143" pad="P13"/>
<connect gate="P" pin="VSS@144" pad="P15"/>
<connect gate="P" pin="VSS@145" pad="P17"/>
<connect gate="P" pin="VSS@146" pad="P19"/>
<connect gate="P" pin="VSS@147" pad="P23"/>
<connect gate="P" pin="VSS@148" pad="P27"/>
<connect gate="P" pin="VSS@149" pad="P5"/>
<connect gate="P" pin="VSS@15" pad="AC10"/>
<connect gate="P" pin="VSS@150" pad="P9"/>
<connect gate="P" pin="VSS@151" pad="R10"/>
<connect gate="P" pin="VSS@152" pad="R12"/>
<connect gate="P" pin="VSS@153" pad="R14"/>
<connect gate="P" pin="VSS@154" pad="R16"/>
<connect gate="P" pin="VSS@155" pad="R18"/>
<connect gate="P" pin="VSS@156" pad="R24"/>
<connect gate="P" pin="VSS@157" pad="T11"/>
<connect gate="P" pin="VSS@158" pad="T13"/>
<connect gate="P" pin="VSS@159" pad="T15"/>
<connect gate="P" pin="VSS@16" pad="AC13"/>
<connect gate="P" pin="VSS@160" pad="T17"/>
<connect gate="P" pin="VSS@161" pad="T19"/>
<connect gate="P" pin="VSS@162" pad="T23"/>
<connect gate="P" pin="VSS@163" pad="T27"/>
<connect gate="P" pin="VSS@164" pad="T5"/>
<connect gate="P" pin="VSS@165" pad="T9"/>
<connect gate="P" pin="VSS@166" pad="U10"/>
<connect gate="P" pin="VSS@167" pad="U12"/>
<connect gate="P" pin="VSS@168" pad="U14"/>
<connect gate="P" pin="VSS@169" pad="U16"/>
<connect gate="P" pin="VSS@17" pad="AC16"/>
<connect gate="P" pin="VSS@170" pad="U18"/>
<connect gate="P" pin="VSS@171" pad="U2"/>
<connect gate="P" pin="VSS@172" pad="U24"/>
<connect gate="P" pin="VSS@173" pad="V11"/>
<connect gate="P" pin="VSS@174" pad="V13"/>
<connect gate="P" pin="VSS@175" pad="V15"/>
<connect gate="P" pin="VSS@176" pad="V17"/>
<connect gate="P" pin="VSS@177" pad="V19"/>
<connect gate="P" pin="VSS@178" pad="V23"/>
<connect gate="P" pin="VSS@179" pad="V27"/>
<connect gate="P" pin="VSS@18" pad="AC19"/>
<connect gate="P" pin="VSS@180" pad="V5"/>
<connect gate="P" pin="VSS@181" pad="V9"/>
<connect gate="P" pin="VSS@182" pad="W10"/>
<connect gate="P" pin="VSS@183" pad="W12"/>
<connect gate="P" pin="VSS@184" pad="W14"/>
<connect gate="P" pin="VSS@185" pad="W16"/>
<connect gate="P" pin="VSS@186" pad="W18"/>
<connect gate="P" pin="VSS@187" pad="Y1"/>
<connect gate="P" pin="VSS@188" pad="Y23"/>
<connect gate="P" pin="VSS@189" pad="Y5"/>
<connect gate="P" pin="VSS@19" pad="AC2"/>
<connect gate="P" pin="VSS@2" pad="A17"/>
<connect gate="P" pin="VSS@20" pad="AC22"/>
<connect gate="P" pin="VSS@21" pad="AC6"/>
<connect gate="P" pin="VSS@22" pad="AC8"/>
<connect gate="P" pin="VSS@23" pad="AD1"/>
<connect gate="P" pin="VSS@24" pad="AD11"/>
<connect gate="P" pin="VSS@25" pad="AD18"/>
<connect gate="P" pin="VSS@26" pad="AD2"/>
<connect gate="P" pin="VSS@27" pad="AD22"/>
<connect gate="P" pin="VSS@28" pad="AE1"/>
<connect gate="P" pin="VSS@29" pad="AE11"/>
<connect gate="P" pin="VSS@3" pad="A2"/>
<connect gate="P" pin="VSS@30" pad="AE12"/>
<connect gate="P" pin="VSS@31" pad="AE15"/>
<connect gate="P" pin="VSS@32" pad="AE16"/>
<connect gate="P" pin="VSS@33" pad="AE2"/>
<connect gate="P" pin="VSS@34" pad="AE20"/>
<connect gate="P" pin="VSS@35" pad="AE3"/>
<connect gate="P" pin="VSS@36" pad="AF1"/>
<connect gate="P" pin="VSS@37" pad="AF11"/>
<connect gate="P" pin="VSS@38" pad="AF14"/>
<connect gate="P" pin="VSS@39" pad="AF18"/>
<connect gate="P" pin="VSS@4" pad="A26"/>
<connect gate="P" pin="VSS@40" pad="AF2"/>
<connect gate="P" pin="VSS@41" pad="AF20"/>
<connect gate="P" pin="VSS@42" pad="AF23"/>
<connect gate="P" pin="VSS@43" pad="AF26"/>
<connect gate="P" pin="VSS@44" pad="AF27"/>
<connect gate="P" pin="VSS@45" pad="AF3"/>
<connect gate="P" pin="VSS@46" pad="AF8"/>
<connect gate="P" pin="VSS@47" pad="AG12"/>
<connect gate="P" pin="VSS@48" pad="AG15"/>
<connect gate="P" pin="VSS@49" pad="AG16"/>
<connect gate="P" pin="VSS@5" pad="A3"/>
<connect gate="P" pin="VSS@50" pad="AG19"/>
<connect gate="P" pin="VSS@51" pad="AG2"/>
<connect gate="P" pin="VSS@52" pad="AG22"/>
<connect gate="P" pin="VSS@53" pad="AG3"/>
<connect gate="P" pin="VSS@54" pad="AG4"/>
<connect gate="P" pin="VSS@55" pad="AG5"/>
<connect gate="P" pin="VSS@56" pad="B1"/>
<connect gate="P" pin="VSS@57" pad="B10"/>
<connect gate="P" pin="VSS@58" pad="B11"/>
<connect gate="P" pin="VSS@59" pad="B14"/>
<connect gate="P" pin="VSS@6" pad="A4"/>
<connect gate="P" pin="VSS@60" pad="B15"/>
<connect gate="P" pin="VSS@61" pad="B16"/>
<connect gate="P" pin="VSS@62" pad="B2"/>
<connect gate="P" pin="VSS@63" pad="B23"/>
<connect gate="P" pin="VSS@64" pad="B3"/>
<connect gate="P" pin="VSS@65" pad="B4"/>
<connect gate="P" pin="VSS@66" pad="B5"/>
<connect gate="P" pin="VSS@67" pad="B6"/>
<connect gate="P" pin="VSS@68" pad="B7"/>
<connect gate="P" pin="VSS@69" pad="B9"/>
<connect gate="P" pin="VSS@7" pad="A6"/>
<connect gate="P" pin="VSS@70" pad="C1"/>
<connect gate="P" pin="VSS@71" pad="C15"/>
<connect gate="P" pin="VSS@72" pad="C18"/>
<connect gate="P" pin="VSS@73" pad="C2"/>
<connect gate="P" pin="VSS@74" pad="C24"/>
<connect gate="P" pin="VSS@75" pad="C3"/>
<connect gate="P" pin="VSS@76" pad="C8"/>
<connect gate="P" pin="VSS@77" pad="D1"/>
<connect gate="P" pin="VSS@78" pad="D10"/>
<connect gate="P" pin="VSS@79" pad="D11"/>
<connect gate="P" pin="VSS@8" pad="A7"/>
<connect gate="P" pin="VSS@80" pad="D13"/>
<connect gate="P" pin="VSS@81" pad="D14"/>
<connect gate="P" pin="VSS@82" pad="D15"/>
<connect gate="P" pin="VSS@83" pad="D16"/>
<connect gate="P" pin="VSS@84" pad="D17"/>
<connect gate="P" pin="VSS@85" pad="D2"/>
<connect gate="P" pin="VSS@86" pad="D23"/>
<connect gate="P" pin="VSS@87" pad="D3"/>
<connect gate="P" pin="VSS@88" pad="D8"/>
<connect gate="P" pin="VSS@89" pad="E10"/>
<connect gate="P" pin="VSS@9" pad="A8"/>
<connect gate="P" pin="VSS@90" pad="E12"/>
<connect gate="P" pin="VSS@91" pad="E14"/>
<connect gate="P" pin="VSS@92" pad="E16"/>
<connect gate="P" pin="VSS@93" pad="E18"/>
<connect gate="P" pin="VSS@94" pad="E2"/>
<connect gate="P" pin="VSS@95" pad="E20"/>
<connect gate="P" pin="VSS@96" pad="E22"/>
<connect gate="P" pin="VSS@97" pad="E26"/>
<connect gate="P" pin="VSS@98" pad="E8"/>
<connect gate="P" pin="VSS@99" pad="F1"/>
<connect gate="P" pin="XWRSTZ" pad="AD5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1791956"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TAS5261" prefix="IC">
<description>&lt;b&gt;315-W Mono BTL Digital Amplifier Power Stage&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tas5261.pdf</description>
<gates>
<gate name="P" symbol="TAS5261"/>
<gate name="EXP" symbol="EXP-3"/>
</gates>
<devices>
<device name="" package="DKD_R-PDSO-G36">
<connects>
<connect gate="EXP" pin="EXP@1" pad="EXP@1"/>
<connect gate="EXP" pin="EXP@2" pad="EXP@2"/>
<connect gate="EXP" pin="EXP@3" pad="EXP@3"/>
<connect gate="P" pin="!OTW" pad="3"/>
<connect gate="P" pin="!RESET" pad="5"/>
<connect gate="P" pin="!SD" pad="4"/>
<connect gate="P" pin="AGND" pad="9"/>
<connect gate="P" pin="BST_A" pad="1"/>
<connect gate="P" pin="BST_B" pad="18"/>
<connect gate="P" pin="GND" pad="8"/>
<connect gate="P" pin="GND@1" pad="16"/>
<connect gate="P" pin="GVDD_A" pad="2"/>
<connect gate="P" pin="GVDD_B" pad="17"/>
<connect gate="P" pin="M1" pad="13"/>
<connect gate="P" pin="M2" pad="12"/>
<connect gate="P" pin="M3" pad="11"/>
<connect gate="P" pin="OC_ADJ" pad="7"/>
<connect gate="P" pin="OUT_A@1" pad="28"/>
<connect gate="P" pin="OUT_A@2" pad="29"/>
<connect gate="P" pin="OUT_A@3" pad="30"/>
<connect gate="P" pin="OUT_B@1" pad="25"/>
<connect gate="P" pin="OUT_B@2" pad="26"/>
<connect gate="P" pin="OUT_B@3" pad="27"/>
<connect gate="P" pin="PGND@1" pad="22"/>
<connect gate="P" pin="PGND@2" pad="23"/>
<connect gate="P" pin="PGND@3" pad="24"/>
<connect gate="P" pin="PGND@4" pad="31"/>
<connect gate="P" pin="PGND@5" pad="32"/>
<connect gate="P" pin="PGND@6" pad="33"/>
<connect gate="P" pin="PVDD_A@1" pad="34"/>
<connect gate="P" pin="PVDD_A@2" pad="35"/>
<connect gate="P" pin="PVDD_A@3" pad="36"/>
<connect gate="P" pin="PVDD_B@1" pad="19"/>
<connect gate="P" pin="PVDD_B@2" pad="20"/>
<connect gate="P" pin="PVDD_B@3" pad="21"/>
<connect gate="P" pin="PWM_A" pad="6"/>
<connect gate="P" pin="PWM_B" pad="14"/>
<connect gate="P" pin="VDD" pad="15"/>
<connect gate="P" pin="VREG" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="TAS5261DKD"/>
<attribute name="OC_FARNELL" value="1564920"/>
<attribute name="OC_NEWARK" value="18M3142"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TL7660" prefix="IC">
<description>&lt;b&gt;CMOS VOLTAGE CONVERTER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/scas794/scas794.pdf</description>
<gates>
<gate name="G$1" symbol="TL7660"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="G$1" pin="CAP+" pad="2"/>
<connect gate="G$1" pin="CAP-" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LV" pad="6"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TL7660CP"/>
<attribute name="OC_FARNELL" value="1755283"/>
<attribute name="OC_NEWARK" value="14M2447"/>
</technology>
</technologies>
</device>
<device name="D" package="D_R-PDSO-G08">
<connects>
<connect gate="G$1" pin="CAP+" pad="2"/>
<connect gate="G$1" pin="CAP-" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LV" pad="6"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TL7660CD"/>
<attribute name="OC_FARNELL" value="1755282"/>
<attribute name="OC_NEWARK" value="14M2439"/>
</technology>
</technologies>
</device>
<device name="DGK" package="DGK_S-PDSO-G8">
<connects>
<connect gate="G$1" pin="CAP+" pad="2"/>
<connect gate="G$1" pin="CAP-" pad="4"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="LV" pad="6"/>
<connect gate="G$1" pin="OSC" pad="7"/>
<connect gate="G$1" pin="VCC" pad="8"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1792" prefix="IC">
<description>&lt;b&gt;24-BIT, 192-kHz SAMPLING, ADVANCED SEGMENT, AUDIO STEREO DIGITAL-TO-ANALOG CONVERTER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm1792.pdf</description>
<gates>
<gate name="G$1" symbol="PCM1792"/>
</gates>
<devices>
<device name="" package="DB_R-PDSO-G28">
<connects>
<connect gate="G$1" pin="!MS" pad="10"/>
<connect gate="G$1" pin="!RST" pad="14"/>
<connect gate="G$1" pin="AGND1" pad="19"/>
<connect gate="G$1" pin="AGND2" pad="24"/>
<connect gate="G$1" pin="AGND3L" pad="27"/>
<connect gate="G$1" pin="AGND3R" pad="16"/>
<connect gate="G$1" pin="BCK" pad="6"/>
<connect gate="G$1" pin="DATA" pad="5"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="IOUTL+" pad="25"/>
<connect gate="G$1" pin="IOUTL-" pad="26"/>
<connect gate="G$1" pin="IOUTR+" pad="17"/>
<connect gate="G$1" pin="IOUTR-" pad="18"/>
<connect gate="G$1" pin="IREF" pad="20"/>
<connect gate="G$1" pin="LRCK" pad="4"/>
<connect gate="G$1" pin="MC" pad="12"/>
<connect gate="G$1" pin="MDI" pad="11"/>
<connect gate="G$1" pin="MDO" pad="13"/>
<connect gate="G$1" pin="MSEL" pad="3"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2L" pad="28"/>
<connect gate="G$1" pin="VCC2R" pad="15"/>
<connect gate="G$1" pin="VCOML" pad="22"/>
<connect gate="G$1" pin="VCOMR" pad="21"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="ZEROL" pad="1"/>
<connect gate="G$1" pin="ZEROR" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PCM1792DB"/>
<attribute name="OC_FARNELL" value="1207081"/>
<attribute name="OC_NEWARK" value="61H5171"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1796" prefix="IC">
<description>&lt;b&gt;24-BIT, 192-kHz SAMPLING, ADVANCED SEGMENT, AUDIO STEREO DIGITAL-TO-ANALOG CONVERTER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm1796.pdf</description>
<gates>
<gate name="G$1" symbol="PCM1792"/>
</gates>
<devices>
<device name="" package="DB_R-PDSO-G28">
<connects>
<connect gate="G$1" pin="!MS" pad="10"/>
<connect gate="G$1" pin="!RST" pad="14"/>
<connect gate="G$1" pin="AGND1" pad="19"/>
<connect gate="G$1" pin="AGND2" pad="24"/>
<connect gate="G$1" pin="AGND3L" pad="27"/>
<connect gate="G$1" pin="AGND3R" pad="16"/>
<connect gate="G$1" pin="BCK" pad="6"/>
<connect gate="G$1" pin="DATA" pad="5"/>
<connect gate="G$1" pin="DGND" pad="8"/>
<connect gate="G$1" pin="IOUTL+" pad="25"/>
<connect gate="G$1" pin="IOUTL-" pad="26"/>
<connect gate="G$1" pin="IOUTR+" pad="17"/>
<connect gate="G$1" pin="IOUTR-" pad="18"/>
<connect gate="G$1" pin="IREF" pad="20"/>
<connect gate="G$1" pin="LRCK" pad="4"/>
<connect gate="G$1" pin="MC" pad="12"/>
<connect gate="G$1" pin="MDI" pad="11"/>
<connect gate="G$1" pin="MDO" pad="13"/>
<connect gate="G$1" pin="MSEL" pad="3"/>
<connect gate="G$1" pin="SCK" pad="7"/>
<connect gate="G$1" pin="VCC1" pad="23"/>
<connect gate="G$1" pin="VCC2L" pad="28"/>
<connect gate="G$1" pin="VCC2R" pad="15"/>
<connect gate="G$1" pin="VCOML" pad="22"/>
<connect gate="G$1" pin="VCOMR" pad="21"/>
<connect gate="G$1" pin="VDD" pad="9"/>
<connect gate="G$1" pin="ZEROL" pad="1"/>
<connect gate="G$1" pin="ZEROR" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM1796DB"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90H2298"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM4220" prefix="IC">
<description>&lt;b&gt;High-Performance, Two-Channel, 24-Bit, 216kHz Sampling Multi-Bit Delta-Sigma Analog-to-Digital Converter&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source:http://focus.ti.com/lit/ds/symlink/pcm4220.pdf</description>
<gates>
<gate name="G$1" symbol="PCM4220"/>
</gates>
<devices>
<device name="X" package="PFB_S-PQFP-G48">
<connects>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="AGND@1" pad="5"/>
<connect gate="G$1" pin="AGND@2" pad="6"/>
<connect gate="G$1" pin="AGND@3" pad="7"/>
<connect gate="G$1" pin="AGND@4" pad="8"/>
<connect gate="G$1" pin="AGND@5" pad="12"/>
<connect gate="G$1" pin="BCK" pad="33"/>
<connect gate="G$1" pin="DATA" pad="32"/>
<connect gate="G$1" pin="DF" pad="21"/>
<connect gate="G$1" pin="DGND" pad="22"/>
<connect gate="G$1" pin="DGND@1" pad="23"/>
<connect gate="G$1" pin="DGND@2" pad="24"/>
<connect gate="G$1" pin="DGND@3" pad="30"/>
<connect gate="G$1" pin="DGND@4" pad="40"/>
<connect gate="G$1" pin="DGND@5" pad="45"/>
<connect gate="G$1" pin="FMT0" pad="44"/>
<connect gate="G$1" pin="FMT1" pad="43"/>
<connect gate="G$1" pin="FS0" pad="19"/>
<connect gate="G$1" pin="FS1" pad="20"/>
<connect gate="G$1" pin="HPFDL" pad="18"/>
<connect gate="G$1" pin="HPFDR" pad="17"/>
<connect gate="G$1" pin="LRCK" pad="34"/>
<connect gate="G$1" pin="MCKI" pad="35"/>
<connect gate="G$1" pin="NC" pad="27"/>
<connect gate="G$1" pin="NC@1" pad="28"/>
<connect gate="G$1" pin="NC@2" pad="29"/>
<connect gate="G$1" pin="OVFL" pad="37"/>
<connect gate="G$1" pin="OVFR" pad="38"/>
<connect gate="G$1" pin="OWL0" pad="42"/>
<connect gate="G$1" pin="OWL1" pad="41"/>
<connect gate="G$1" pin="PCMEN" pad="16"/>
<connect gate="G$1" pin="REFGNDL" pad="14"/>
<connect gate="G$1" pin="REFGNDR" pad="47"/>
<connect gate="G$1" pin="RST" pad="36"/>
<connect gate="G$1" pin="S/M" pad="39"/>
<connect gate="G$1" pin="SUB0" pad="26"/>
<connect gate="G$1" pin="SUB1" pad="25"/>
<connect gate="G$1" pin="VCC1" pad="4"/>
<connect gate="G$1" pin="VCC2" pad="9"/>
<connect gate="G$1" pin="VCOML" pad="13"/>
<connect gate="G$1" pin="VCOMR" pad="48"/>
<connect gate="G$1" pin="VDD" pad="31"/>
<connect gate="G$1" pin="VINL+" pad="11"/>
<connect gate="G$1" pin="VINL-" pad="10"/>
<connect gate="G$1" pin="VINR+" pad="3"/>
<connect gate="G$1" pin="VINR-" pad="2"/>
<connect gate="G$1" pin="VREFL" pad="15"/>
<connect gate="G$1" pin="VREFR" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCM4220PFB"/>
<attribute name="OC_FARNELL" value="1754967"/>
<attribute name="OC_NEWARK" value="46M6821"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM4222" prefix="IC">
<description>&lt;b&gt;High-Performance, Two-Channel, 24-Bit, 216kHz Sampling Multi-Bit Delta-Sigma Analog-to-Digital Converter&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm4222.pdf</description>
<gates>
<gate name="G$1" symbol="PCM4222"/>
</gates>
<devices>
<device name="" package="PFB_S-PQFP-G48">
<connects>
<connect gate="G$1" pin="AGND" pad="1"/>
<connect gate="G$1" pin="AGND@1" pad="5"/>
<connect gate="G$1" pin="AGND@2" pad="6"/>
<connect gate="G$1" pin="AGND@3" pad="7"/>
<connect gate="G$1" pin="AGND@4" pad="8"/>
<connect gate="G$1" pin="AGND@5" pad="12"/>
<connect gate="G$1" pin="BCK" pad="33"/>
<connect gate="G$1" pin="DATA" pad="32"/>
<connect gate="G$1" pin="DF/MOD5" pad="21"/>
<connect gate="G$1" pin="DGND" pad="30"/>
<connect gate="G$1" pin="DGND@1" pad="40"/>
<connect gate="G$1" pin="DGND@2" pad="45"/>
<connect gate="G$1" pin="DSDCLK" pad="27"/>
<connect gate="G$1" pin="DSDEN/MOD6" pad="22"/>
<connect gate="G$1" pin="DSDL" pad="28"/>
<connect gate="G$1" pin="DSDMODE" pad="24"/>
<connect gate="G$1" pin="DSDR" pad="29"/>
<connect gate="G$1" pin="FMT0" pad="44"/>
<connect gate="G$1" pin="FMT1" pad="43"/>
<connect gate="G$1" pin="FS0/MOD3" pad="19"/>
<connect gate="G$1" pin="FS1/MOD4" pad="20"/>
<connect gate="G$1" pin="HPFDL/MOD2" pad="18"/>
<connect gate="G$1" pin="HPFDR/MOD1" pad="17"/>
<connect gate="G$1" pin="LRCK" pad="34"/>
<connect gate="G$1" pin="MCKI" pad="35"/>
<connect gate="G$1" pin="MODEN" pad="23"/>
<connect gate="G$1" pin="OVFL" pad="37"/>
<connect gate="G$1" pin="OVFR" pad="38"/>
<connect gate="G$1" pin="OWL0" pad="42"/>
<connect gate="G$1" pin="OWL1" pad="41"/>
<connect gate="G$1" pin="PCMEN" pad="16"/>
<connect gate="G$1" pin="REFGNDL" pad="14"/>
<connect gate="G$1" pin="REFGNDR" pad="47"/>
<connect gate="G$1" pin="RST" pad="36"/>
<connect gate="G$1" pin="S/M" pad="39"/>
<connect gate="G$1" pin="SUB0/WCKO" pad="26"/>
<connect gate="G$1" pin="SUB1/MCKO" pad="25"/>
<connect gate="G$1" pin="VCC1" pad="4"/>
<connect gate="G$1" pin="VCC2" pad="9"/>
<connect gate="G$1" pin="VCOML" pad="13"/>
<connect gate="G$1" pin="VCOMR" pad="48"/>
<connect gate="G$1" pin="VDD" pad="31"/>
<connect gate="G$1" pin="VIN-" pad="2"/>
<connect gate="G$1" pin="VINL+" pad="11"/>
<connect gate="G$1" pin="VINL-" pad="10"/>
<connect gate="G$1" pin="VINR+" pad="3"/>
<connect gate="G$1" pin="VREFL" pad="15"/>
<connect gate="G$1" pin="VREFR" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PCM4222PFB"/>
<attribute name="OC_FARNELL" value="1390708"/>
<attribute name="OC_NEWARK" value="36M9296"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM4204" prefix="IC">
<description>&lt;b&gt;High-Performance 24-Bit, 216kHz Sampling Four-Channel Audio-to-Digital Converter&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm4204.pdf</description>
<gates>
<gate name="G$1" symbol="PCM4204"/>
</gates>
<devices>
<device name="" package="PAP_S-PQFP-G64">
<connects>
<connect gate="G$1" pin="AGND1" pad="6"/>
<connect gate="G$1" pin="AGND2" pad="43"/>
<connect gate="G$1" pin="AGND3" pad="51"/>
<connect gate="G$1" pin="AGND4" pad="62"/>
<connect gate="G$1" pin="BCK" pad="29"/>
<connect gate="G$1" pin="BGND1" pad="7"/>
<connect gate="G$1" pin="BGND2" pad="16"/>
<connect gate="G$1" pin="BGND3" pad="33"/>
<connect gate="G$1" pin="BGND4" pad="42"/>
<connect gate="G$1" pin="CLIP1" pad="34"/>
<connect gate="G$1" pin="CLIP2" pad="35"/>
<connect gate="G$1" pin="CLIP3" pad="36"/>
<connect gate="G$1" pin="CLIP4" pad="37"/>
<connect gate="G$1" pin="DGND1" pad="8"/>
<connect gate="G$1" pin="DGND2" pad="22"/>
<connect gate="G$1" pin="DGND3" pad="41"/>
<connect gate="G$1" pin="DSD1" pad="25"/>
<connect gate="G$1" pin="DSD2" pad="26"/>
<connect gate="G$1" pin="DSD3" pad="27"/>
<connect gate="G$1" pin="DSD4" pad="28"/>
<connect gate="G$1" pin="DSDCLK" pad="24"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="FMT0" pad="18"/>
<connect gate="G$1" pin="FMT1" pad="19"/>
<connect gate="G$1" pin="FMT2" pad="20"/>
<connect gate="G$1" pin="FS0" pad="12"/>
<connect gate="G$1" pin="FS1" pad="13"/>
<connect gate="G$1" pin="FS2" pad="14"/>
<connect gate="G$1" pin="HPFD" pad="38"/>
<connect gate="G$1" pin="LRCK" pad="30"/>
<connect gate="G$1" pin="NC" pad="3"/>
<connect gate="G$1" pin="NC@1" pad="4"/>
<connect gate="G$1" pin="NC@2" pad="21"/>
<connect gate="G$1" pin="NC@3" pad="45"/>
<connect gate="G$1" pin="NC@4" pad="46"/>
<connect gate="G$1" pin="NC@5" pad="53"/>
<connect gate="G$1" pin="NC@6" pad="56"/>
<connect gate="G$1" pin="NC@7" pad="57"/>
<connect gate="G$1" pin="NC@8" pad="60"/>
<connect gate="G$1" pin="RST" pad="10"/>
<connect gate="G$1" pin="S/M" pad="17"/>
<connect gate="G$1" pin="SCKI" pad="15"/>
<connect gate="G$1" pin="SDOUT1" pad="31"/>
<connect gate="G$1" pin="SDOUT2" pad="32"/>
<connect gate="G$1" pin="SUB" pad="39"/>
<connect gate="G$1" pin="TEST" pad="11"/>
<connect gate="G$1" pin="VCC1" pad="5"/>
<connect gate="G$1" pin="VCC2" pad="44"/>
<connect gate="G$1" pin="VCOM12" pad="61"/>
<connect gate="G$1" pin="VCOM34" pad="52"/>
<connect gate="G$1" pin="VDD1" pad="9"/>
<connect gate="G$1" pin="VDD2" pad="23"/>
<connect gate="G$1" pin="VDD3" pad="40"/>
<connect gate="G$1" pin="VIN1+" pad="2"/>
<connect gate="G$1" pin="VIN1-" pad="1"/>
<connect gate="G$1" pin="VIN2+" pad="59"/>
<connect gate="G$1" pin="VIN2-" pad="58"/>
<connect gate="G$1" pin="VIN3+" pad="55"/>
<connect gate="G$1" pin="VIN3-" pad="54"/>
<connect gate="G$1" pin="VIN4+" pad="48"/>
<connect gate="G$1" pin="VIN4-" pad="47"/>
<connect gate="G$1" pin="VREF12+" pad="64"/>
<connect gate="G$1" pin="VREF12-" pad="63"/>
<connect gate="G$1" pin="VREF34+" pad="49"/>
<connect gate="G$1" pin="VREF34-" pad="50"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="PCM4204PAPT"/>
<attribute name="OC_FARNELL" value="9969098"/>
<attribute name="OC_NEWARK" value="43J9723"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCM1804" prefix="IC">
<description>&lt;b&gt;FULL DIFFERENTIAL ANALOG INPUT 24-BIT, 192-kHz STEREO A/D CONVERTER&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 29&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/pcm1804.pdf</description>
<gates>
<gate name="G$1" symbol="PCM1804"/>
</gates>
<devices>
<device name="" package="DB_R-PDSO-G28">
<connects>
<connect gate="G$1" pin="!RST" pad="19"/>
<connect gate="G$1" pin="AGND" pad="23"/>
<connect gate="G$1" pin="AGNDL" pad="2"/>
<connect gate="G$1" pin="AGNDR" pad="27"/>
<connect gate="G$1" pin="BCK/DSDL" pad="16"/>
<connect gate="G$1" pin="BYPAS" pad="12"/>
<connect gate="G$1" pin="DATA/DSDR" pad="15"/>
<connect gate="G$1" pin="DGND" pad="13"/>
<connect gate="G$1" pin="FMT0" pad="6"/>
<connect gate="G$1" pin="FMT1" pad="7"/>
<connect gate="G$1" pin="LRCK/DSDBCK" pad="17"/>
<connect gate="G$1" pin="OSR0" pad="9"/>
<connect gate="G$1" pin="OSR1" pad="10"/>
<connect gate="G$1" pin="OSR2" pad="11"/>
<connect gate="G$1" pin="OVFL" pad="21"/>
<connect gate="G$1" pin="OVFR" pad="20"/>
<connect gate="G$1" pin="S/!M" pad="8"/>
<connect gate="G$1" pin="SCKI" pad="18"/>
<connect gate="G$1" pin="VCC" pad="22"/>
<connect gate="G$1" pin="VCOML" pad="3"/>
<connect gate="G$1" pin="VCOMR" pad="26"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VINL+" pad="4"/>
<connect gate="G$1" pin="VINL-" pad="5"/>
<connect gate="G$1" pin="VINR+" pad="25"/>
<connect gate="G$1" pin="VINR-" pad="24"/>
<connect gate="G$1" pin="VREFL" pad="1"/>
<connect gate="G$1" pin="VREFR" pad="28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="PCM1804DB"/>
<attribute name="OC_FARNELL" value="1197425"/>
<attribute name="OC_NEWARK" value="36K7583"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN65LVD*125" prefix="IC">
<description>&lt;b&gt;LVDS 4x4 CROSSPOINT SWITCH&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn65lvds125a.pdf</description>
<gates>
<gate name="G$1" symbol="SN65LVDS125A"/>
<gate name="P" symbol="VCC4-GND6"/>
</gates>
<devices>
<device name="A" package="DBT_R-PDSO-G38">
<connects>
<connect gate="G$1" pin="1A" pad="3"/>
<connect gate="G$1" pin="1B" pad="4"/>
<connect gate="G$1" pin="1DE" pad="34"/>
<connect gate="G$1" pin="1Y" pad="36"/>
<connect gate="G$1" pin="1Z" pad="35"/>
<connect gate="G$1" pin="2A" pad="7"/>
<connect gate="G$1" pin="2B" pad="8"/>
<connect gate="G$1" pin="2DE" pad="31"/>
<connect gate="G$1" pin="2Y" pad="33"/>
<connect gate="G$1" pin="2Z" pad="32"/>
<connect gate="G$1" pin="3A" pad="12"/>
<connect gate="G$1" pin="3B" pad="13"/>
<connect gate="G$1" pin="3DE" pad="25"/>
<connect gate="G$1" pin="3Y" pad="27"/>
<connect gate="G$1" pin="3Z" pad="26"/>
<connect gate="G$1" pin="4A" pad="16"/>
<connect gate="G$1" pin="4B" pad="17"/>
<connect gate="G$1" pin="4DE" pad="22"/>
<connect gate="G$1" pin="4Y" pad="24"/>
<connect gate="G$1" pin="4Z" pad="23"/>
<connect gate="G$1" pin="S10" pad="1"/>
<connect gate="G$1" pin="S11" pad="2"/>
<connect gate="G$1" pin="S20" pad="5"/>
<connect gate="G$1" pin="S21" pad="6"/>
<connect gate="G$1" pin="S30" pad="14"/>
<connect gate="G$1" pin="S31" pad="15"/>
<connect gate="G$1" pin="S40" pad="18"/>
<connect gate="G$1" pin="S41" pad="19"/>
<connect gate="P" pin="GND@1" pad="9"/>
<connect gate="P" pin="GND@2" pad="11"/>
<connect gate="P" pin="GND@3" pad="21"/>
<connect gate="P" pin="GND@4" pad="28"/>
<connect gate="P" pin="GND@5" pad="30"/>
<connect gate="P" pin="GND@6" pad="37"/>
<connect gate="P" pin="VCC@1" pad="10"/>
<connect gate="P" pin="VCC@2" pad="20"/>
<connect gate="P" pin="VCC@3" pad="29"/>
<connect gate="P" pin="VCC@4" pad="38"/>
</connects>
<technologies>
<technology name="S">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="SN65LVDS125ADBT"/>
<attribute name="OC_FARNELL" value="1408802"/>
<attribute name="OC_NEWARK" value="01J0701"/>
</technology>
<technology name="T">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="SN65LVDT125ADBTR"/>
<attribute name="OC_FARNELL" value="1408842"/>
<attribute name="OC_NEWARK" value="01J0706"/>
</technology>
</technologies>
</device>
<device name="" package="DBT_R-PDSO-G38">
<connects>
<connect gate="G$1" pin="1A" pad="3"/>
<connect gate="G$1" pin="1B" pad="4"/>
<connect gate="G$1" pin="1DE" pad="34"/>
<connect gate="G$1" pin="1Y" pad="36"/>
<connect gate="G$1" pin="1Z" pad="35"/>
<connect gate="G$1" pin="2A" pad="7"/>
<connect gate="G$1" pin="2B" pad="8"/>
<connect gate="G$1" pin="2DE" pad="31"/>
<connect gate="G$1" pin="2Y" pad="33"/>
<connect gate="G$1" pin="2Z" pad="32"/>
<connect gate="G$1" pin="3A" pad="12"/>
<connect gate="G$1" pin="3B" pad="13"/>
<connect gate="G$1" pin="3DE" pad="25"/>
<connect gate="G$1" pin="3Y" pad="27"/>
<connect gate="G$1" pin="3Z" pad="26"/>
<connect gate="G$1" pin="4A" pad="16"/>
<connect gate="G$1" pin="4B" pad="17"/>
<connect gate="G$1" pin="4DE" pad="22"/>
<connect gate="G$1" pin="4Y" pad="24"/>
<connect gate="G$1" pin="4Z" pad="23"/>
<connect gate="G$1" pin="S10" pad="1"/>
<connect gate="G$1" pin="S11" pad="2"/>
<connect gate="G$1" pin="S20" pad="5"/>
<connect gate="G$1" pin="S21" pad="6"/>
<connect gate="G$1" pin="S30" pad="14"/>
<connect gate="G$1" pin="S31" pad="15"/>
<connect gate="G$1" pin="S40" pad="18"/>
<connect gate="G$1" pin="S41" pad="19"/>
<connect gate="P" pin="GND@1" pad="9"/>
<connect gate="P" pin="GND@2" pad="11"/>
<connect gate="P" pin="GND@3" pad="21"/>
<connect gate="P" pin="GND@4" pad="28"/>
<connect gate="P" pin="GND@5" pad="30"/>
<connect gate="P" pin="GND@6" pad="37"/>
<connect gate="P" pin="VCC@1" pad="10"/>
<connect gate="P" pin="VCC@2" pad="20"/>
<connect gate="P" pin="VCC@3" pad="29"/>
<connect gate="P" pin="VCC@4" pad="38"/>
</connects>
<technologies>
<technology name="S">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="SN65LVDS125ADBT"/>
<attribute name="OC_FARNELL" value="1509804"/>
<attribute name="OC_NEWARK" value="01J0701"/>
</technology>
<technology name="T">
<attribute name="MF" value="TEXAS INSTRUMENT CONNECTORS"/>
<attribute name="MPN" value="SN65LVDT125ADBT"/>
<attribute name="OC_FARNELL" value="1408842"/>
<attribute name="OC_NEWARK" value="01J0705"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS1274" prefix="IC">
<description>&lt;b&gt;Quad/Octal, Simultaneous Sampling, 24-Bit Analog-to-Digital Converters&lt;/b&gt; ADS1274 / ADS1278 &lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ads1274.pdf</description>
<gates>
<gate name="G$1" symbol="ADS1274"/>
<gate name="P" symbol="EXP25"/>
</gates>
<devices>
<device name="" package="HTQFP-64-PAP">
<connects>
<connect gate="G$1" pin="!DRDY!/FSYNC" pad="29"/>
<connect gate="G$1" pin="!PWDN1" pad="42"/>
<connect gate="G$1" pin="!PWDN2" pad="41"/>
<connect gate="G$1" pin="!PWDN3" pad="40"/>
<connect gate="G$1" pin="!PWDN4" pad="39"/>
<connect gate="G$1" pin="!PWDN5" pad="38"/>
<connect gate="G$1" pin="!PWDN6" pad="37"/>
<connect gate="G$1" pin="!PWDN7" pad="36"/>
<connect gate="G$1" pin="!PWDN8" pad="35"/>
<connect gate="G$1" pin="!SYNC" pad="11"/>
<connect gate="G$1" pin="AGND" pad="6"/>
<connect gate="G$1" pin="AGND@1" pad="43"/>
<connect gate="G$1" pin="AGND@2" pad="54"/>
<connect gate="G$1" pin="AGND@3" pad="58"/>
<connect gate="G$1" pin="AGND@4" pad="59"/>
<connect gate="G$1" pin="AINN1" pad="4"/>
<connect gate="G$1" pin="AINN2" pad="2"/>
<connect gate="G$1" pin="AINN3" pad="64"/>
<connect gate="G$1" pin="AINN4" pad="62"/>
<connect gate="G$1" pin="AINP1" pad="3"/>
<connect gate="G$1" pin="AINP2" pad="1"/>
<connect gate="G$1" pin="AINP3" pad="63"/>
<connect gate="G$1" pin="AINP4" pad="61"/>
<connect gate="G$1" pin="AVDD" pad="5"/>
<connect gate="G$1" pin="AVDD@1" pad="44"/>
<connect gate="G$1" pin="AVDD@2" pad="53"/>
<connect gate="G$1" pin="AVDD@3" pad="60"/>
<connect gate="G$1" pin="CLK" pad="27"/>
<connect gate="G$1" pin="CLKDIV" pad="10"/>
<connect gate="G$1" pin="DGND" pad="7"/>
<connect gate="G$1" pin="DGND@1" pad="21"/>
<connect gate="G$1" pin="DGND@2" pad="24"/>
<connect gate="G$1" pin="DGND@3" pad="25"/>
<connect gate="G$1" pin="DIN" pad="12"/>
<connect gate="G$1" pin="DOUT1" pad="20"/>
<connect gate="G$1" pin="DOUT2" pad="19"/>
<connect gate="G$1" pin="DOUT3" pad="18"/>
<connect gate="G$1" pin="DOUT4" pad="17"/>
<connect gate="G$1" pin="DOUT5" pad="16"/>
<connect gate="G$1" pin="DOUT6" pad="15"/>
<connect gate="G$1" pin="DOUT7" pad="14"/>
<connect gate="G$1" pin="DOUT8" pad="13"/>
<connect gate="G$1" pin="DVDD" pad="26"/>
<connect gate="G$1" pin="EDS@1" pad="52"/>
<connect gate="G$1" pin="EDS@2" pad="50"/>
<connect gate="G$1" pin="EDS@3" pad="48"/>
<connect gate="G$1" pin="EDS@4" pad="46"/>
<connect gate="G$1" pin="EDS@5" pad="51"/>
<connect gate="G$1" pin="EDS@6" pad="49"/>
<connect gate="G$1" pin="EDS@7" pad="47"/>
<connect gate="G$1" pin="EDS@8" pad="45"/>
<connect gate="G$1" pin="FORMAT0" pad="32"/>
<connect gate="G$1" pin="FORMAT1" pad="31"/>
<connect gate="G$1" pin="FORMAT2" pad="30"/>
<connect gate="G$1" pin="IOVDD" pad="22"/>
<connect gate="G$1" pin="IOVDD@1" pad="23"/>
<connect gate="G$1" pin="MODE0" pad="34"/>
<connect gate="G$1" pin="MODE1" pad="33"/>
<connect gate="G$1" pin="SCLK" pad="28"/>
<connect gate="G$1" pin="TEST0" pad="8"/>
<connect gate="G$1" pin="TEST1" pad="9"/>
<connect gate="G$1" pin="VCOM" pad="55"/>
<connect gate="G$1" pin="VREFN" pad="57"/>
<connect gate="G$1" pin="VREFP" pad="56"/>
<connect gate="P" pin="EXP@1" pad="EXP1"/>
<connect gate="P" pin="EXP@10" pad="EXP10"/>
<connect gate="P" pin="EXP@11" pad="EXP11"/>
<connect gate="P" pin="EXP@12" pad="EXP12"/>
<connect gate="P" pin="EXP@13" pad="EXP13"/>
<connect gate="P" pin="EXP@14" pad="EXP14"/>
<connect gate="P" pin="EXP@15" pad="EXP15"/>
<connect gate="P" pin="EXP@16" pad="EXP16"/>
<connect gate="P" pin="EXP@17" pad="EXP17"/>
<connect gate="P" pin="EXP@18" pad="EXP18"/>
<connect gate="P" pin="EXP@19" pad="EXP19"/>
<connect gate="P" pin="EXP@2" pad="EXP2"/>
<connect gate="P" pin="EXP@20" pad="EXP20"/>
<connect gate="P" pin="EXP@21" pad="EXP21"/>
<connect gate="P" pin="EXP@22" pad="EXP22"/>
<connect gate="P" pin="EXP@23" pad="EXP23"/>
<connect gate="P" pin="EXP@24" pad="EXP24"/>
<connect gate="P" pin="EXP@25" pad="EXP25"/>
<connect gate="P" pin="EXP@3" pad="EXP3"/>
<connect gate="P" pin="EXP@4" pad="EXP4"/>
<connect gate="P" pin="EXP@5" pad="EXP5"/>
<connect gate="P" pin="EXP@6" pad="EXP6"/>
<connect gate="P" pin="EXP@7" pad="EXP7"/>
<connect gate="P" pin="EXP@8" pad="EXP8"/>
<connect gate="P" pin="EXP@9" pad="EXP9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ADS1274IPAPT"/>
<attribute name="OC_FARNELL" value="1603418"/>
<attribute name="OC_NEWARK" value="50M8809"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OMAP-L138ZWT" prefix="IC">
<description>&lt;b&gt;OMAP-L138 Low-Power Applications Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Source: sprm376a.bsm&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/omap-l138.pdf&lt;br&gt;&lt;i&gt;Connect-List generated from &lt;/i&gt;&lt;b&gt;OMAPL138ZWT.DEV&lt;/b&gt; Variant &lt;b&gt;''&lt;/b&gt; with &lt;i&gt;&lt;b&gt;connect-device-split-symbol-03.ulp&lt;/b&gt;&lt;/i&gt;</description>
<gates>
<gate name="A" symbol="OMAPL138Z-A"/>
<gate name="B" symbol="OMAPL138Z-B"/>
<gate name="C" symbol="OMAPL138Z-C"/>
<gate name="D" symbol="OMAPL138Z-D"/>
<gate name="E" symbol="OMAPL138Z-E"/>
<gate name="P" symbol="OMAPL138Z-P"/>
</gates>
<devices>
<device name="" package="ZWT_S-PBGA-N361">
<connects>
<connect gate="A" pin="ACLKR_GP015" pad="A1"/>
<connect gate="A" pin="ACLKX_GP014" pad="B1"/>
<connect gate="A" pin="AFSR0_GP013" pad="C2"/>
<connect gate="A" pin="AFSX0_GP012" pad="B2"/>
<connect gate="A" pin="AHCLKR_UART1RTS_GP011" pad="A2"/>
<connect gate="A" pin="AHCLKX_USBREFCLKIN_UART1CTS_GP010" pad="A3"/>
<connect gate="A" pin="AMUTEIN_RTCALARM_UART2CTS_GP08_DEEPSLEEPN" pad="F4"/>
<connect gate="A" pin="AMUTE_UART2RTS_GP09" pad="D5"/>
<connect gate="A" pin="AXR00_ECAP0APWM0_GP87_MIITXD0_CLKS0" pad="F3"/>
<connect gate="A" pin="AXR010_DR1_GP02" pad="D4"/>
<connect gate="A" pin="AXR011_FSX1_GP03" pad="C5"/>
<connect gate="A" pin="AXR012_FSR1_GP04" pad="C4"/>
<connect gate="A" pin="AXR013_CLKX1_GP05" pad="B3"/>
<connect gate="A" pin="AXR014_CLKR1_GP06" pad="B4"/>
<connect gate="A" pin="AXR015_EPWM0TZ0_ECAP2APWM2_GP07" pad="A4"/>
<connect gate="A" pin="AXR01_DX0_GP19MIITXD1" pad="E1"/>
<connect gate="A" pin="AXR02_DR0_GP110_MIITXD2" pad="E2"/>
<connect gate="A" pin="AXR03_FSX0_GP111_MIITXD3" pad="E3"/>
<connect gate="A" pin="AXR04_FSR0_GP112_MIICOL" pad="D1"/>
<connect gate="A" pin="AXR05_CLKX0_GP113_MIITXCLK" pad="D3"/>
<connect gate="A" pin="AXR06_CLKR0_GP114_MIITXEN" pad="C1"/>
<connect gate="A" pin="AXR07_EPWM1TZ0_GP115" pad="D2"/>
<connect gate="A" pin="AXR08_CLKS1_ECAP1APWM1_GP00" pad="E4"/>
<connect gate="A" pin="AXR09_DX1_GP01" pad="C3"/>
<connect gate="A" pin="CLKOUT_UHPIHDS2N_GP614" pad="T18"/>
<connect gate="B" pin="DDRA0" pad="U7"/>
<connect gate="B" pin="DDRA1" pad="T7"/>
<connect gate="B" pin="DDRA10" pad="W4"/>
<connect gate="B" pin="DDRA11" pad="T4"/>
<connect gate="B" pin="DDRA12" pad="V4"/>
<connect gate="B" pin="DDRA13" pad="T5"/>
<connect gate="B" pin="DDRA2" pad="W6"/>
<connect gate="B" pin="DDRA3" pad="V6"/>
<connect gate="B" pin="DDRA4" pad="U5"/>
<connect gate="B" pin="DDRA5" pad="V5"/>
<connect gate="B" pin="DDRA6" pad="W5"/>
<connect gate="B" pin="DDRA7" pad="U6"/>
<connect gate="B" pin="DDRA8" pad="U4"/>
<connect gate="B" pin="DDRA9" pad="T6"/>
<connect gate="B" pin="DDRBA0" pad="V8"/>
<connect gate="B" pin="DDRBA1" pad="T9"/>
<connect gate="B" pin="DDRBA2" pad="U8"/>
<connect gate="B" pin="DDRCASN" pad="U9"/>
<connect gate="B" pin="DDRCKE" pad="V7"/>
<connect gate="B" pin="DDRCLKN" pad="W7"/>
<connect gate="B" pin="DDRCLKP" pad="W8"/>
<connect gate="B" pin="DDRCSN" pad="V9"/>
<connect gate="B" pin="DDRD0" pad="U15"/>
<connect gate="B" pin="DDRD1" pad="U14"/>
<connect gate="B" pin="DDRD10" pad="T10"/>
<connect gate="B" pin="DDRD11" pad="T12"/>
<connect gate="B" pin="DDRD12" pad="U10"/>
<connect gate="B" pin="DDRD13" pad="V10"/>
<connect gate="B" pin="DDRD14" pad="U11"/>
<connect gate="B" pin="DDRD15" pad="W10"/>
<connect gate="B" pin="DDRD2" pad="V14"/>
<connect gate="B" pin="DDRD3" pad="U13"/>
<connect gate="B" pin="DDRD4" pad="V13"/>
<connect gate="B" pin="DDRD5" pad="V12"/>
<connect gate="B" pin="DDRD6" pad="W12"/>
<connect gate="B" pin="DDRD7" pad="W11"/>
<connect gate="B" pin="DDRD8" pad="T13"/>
<connect gate="B" pin="DDRD9" pad="T11"/>
<connect gate="B" pin="DDRDQGATE0" pad="R11"/>
<connect gate="B" pin="DDRDQGATE1" pad="R12"/>
<connect gate="B" pin="DDRDQM0N" pad="W13"/>
<connect gate="B" pin="DDRDQM1N" pad="R10"/>
<connect gate="B" pin="DDRDQS0" pad="T14"/>
<connect gate="B" pin="DDRDQS1" pad="V11"/>
<connect gate="B" pin="DDRRASN" pad="W9"/>
<connect gate="B" pin="DDRWEN" pad="T8"/>
<connect gate="C" pin="EMAA0_GP50" pad="C14"/>
<connect gate="C" pin="EMAA10_GP510" pad="C12"/>
<connect gate="C" pin="EMAA11_GP511" pad="B12"/>
<connect gate="C" pin="EMAA12_GP512" pad="D13"/>
<connect gate="C" pin="EMAA13_GP513" pad="D11"/>
<connect gate="C" pin="EMAA14_MMCSD0DAT7_GP514" pad="A12"/>
<connect gate="C" pin="EMAA15_MMCSD0DAT6_GP515" pad="C11"/>
<connect gate="C" pin="EMAA16_MMCSD0DAT5_GP40" pad="E12"/>
<connect gate="C" pin="EMAA17_MMCSD0DAT4_GP41" pad="B11"/>
<connect gate="C" pin="EMAA18_MMCSD0DAT3_GP42" pad="E11"/>
<connect gate="C" pin="EMAA19_MMCSD0DAT2_GP43" pad="C10"/>
<connect gate="C" pin="EMAA1_GP51" pad="D15"/>
<connect gate="C" pin="EMAA20_MMCSD0DAT1_GP44" pad="A11"/>
<connect gate="C" pin="EMAA21_MMCSD0DAT0_GP45" pad="B10"/>
<connect gate="C" pin="EMAA22_MMCSD0CMD_GP46" pad="A10"/>
<connect gate="C" pin="EMAA23_MMCSD0CLK_GP47" pad="E9"/>
<connect gate="C" pin="EMAA2_GP52" pad="B14"/>
<connect gate="C" pin="EMAA3_GP53" pad="D14"/>
<connect gate="C" pin="EMAA4_GP54" pad="A14"/>
<connect gate="C" pin="EMAA5_GP55" pad="C13"/>
<connect gate="C" pin="EMAA6_GP56" pad="E13"/>
<connect gate="C" pin="EMAA7_GP57" pad="B13"/>
<connect gate="C" pin="EMAA8_GP58" pad="A13"/>
<connect gate="C" pin="EMAA9_GP59" pad="D12"/>
<connect gate="C" pin="EMABA0_GP28" pad="C15"/>
<connect gate="C" pin="EMABA1_GP29" pad="A15"/>
<connect gate="C" pin="EMACASN_GP24" pad="A9"/>
<connect gate="C" pin="EMACLK_GP27" pad="B7"/>
<connect gate="C" pin="EMACS0N_GP20" pad="A18"/>
<connect gate="C" pin="EMACS2N_GP315" pad="B17"/>
<connect gate="C" pin="EMACS3N_GP314" pad="A17"/>
<connect gate="C" pin="EMACS4N_GP313" pad="F9"/>
<connect gate="C" pin="EMACS5N_GP212" pad="B16"/>
<connect gate="C" pin="EMAD0_GP48" pad="C9"/>
<connect gate="C" pin="EMAD10_GP32" pad="A7"/>
<connect gate="C" pin="EMAD11_GP33" pad="D6"/>
<connect gate="C" pin="EMAD12_GP34" pad="A6"/>
<connect gate="C" pin="EMAD13_GP35" pad="B6"/>
<connect gate="C" pin="EMAD14_GP36" pad="C7"/>
<connect gate="C" pin="EMAD15_GP37" pad="E6"/>
<connect gate="C" pin="EMAD1_GP49" pad="A8"/>
<connect gate="C" pin="EMAD2_GP410" pad="B8"/>
<connect gate="C" pin="EMAD3_GP411" pad="E8"/>
<connect gate="C" pin="EMAD4_GP412" pad="B5"/>
<connect gate="C" pin="EMAD5_GP413" pad="E7"/>
<connect gate="C" pin="EMAD6_GP414" pad="C6"/>
<connect gate="C" pin="EMAD7_GP415" pad="D7"/>
<connect gate="C" pin="EMAD8_GP30" pad="E10"/>
<connect gate="C" pin="EMAD9_GP31" pad="D9"/>
<connect gate="C" pin="EMAOEN_GP310" pad="B15"/>
<connect gate="C" pin="EMARASN_GP25" pad="A16"/>
<connect gate="C" pin="EMARNW_GP39" pad="D10"/>
<connect gate="C" pin="EMASDCKE_GP26" pad="D8"/>
<connect gate="C" pin="EMAWAIT0_GP38" pad="B18"/>
<connect gate="C" pin="EMAWAIT1_GP21" pad="B19"/>
<connect gate="C" pin="EMAWEDQM0N_GP23" pad="C8"/>
<connect gate="C" pin="EMAWEDQM1N_GP22" pad="A5"/>
<connect gate="C" pin="EMAWEN_GP311" pad="B9"/>
<connect gate="C" pin="EMU0" pad="J16"/>
<connect gate="C" pin="EMU1" pad="K16"/>
<connect gate="D" pin="LCDACENBCSN_GP60" pad="R5"/>
<connect gate="D" pin="MMCSD1CLK_UPPCHBSTART_GP814" pad="G2"/>
<connect gate="D" pin="MMCSD1CMD_UPPCHBENABLE_GP813" pad="J4"/>
<connect gate="D" pin="MMCSD1DAT0_UPPCHBCLOCK_GP815" pad="G1"/>
<connect gate="D" pin="MMCSD1DAT4_LCDVSYNC_GP88" pad="G4"/>
<connect gate="D" pin="MMCSD1DAT5_LCDHSYNC_GP89" pad="H4"/>
<connect gate="D" pin="MMCSD1DAT6_LCDMCLK_GP810" pad="F2"/>
<connect gate="D" pin="MMCSD1DAT7_LCDPCLK_GP811" pad="F1"/>
<connect gate="D" pin="NMIN" pad="J17"/>
<connect gate="D" pin="RESETN" pad="K14"/>
<connect gate="D" pin="RESETOUTN_UHPIHASN_GP615" pad="T17"/>
<connect gate="D" pin="SATARXN" pad="L2"/>
<connect gate="D" pin="SATARXP" pad="L1"/>
<connect gate="D" pin="SATATXP" pad="J1"/>
<connect gate="D" pin="SPI0CLK_EPWM0A_GP18_MIIRXCLK" pad="D19"/>
<connect gate="D" pin="SPI0ENAN_EPWM0B_MIIRXDV" pad="C17"/>
<connect gate="D" pin="SPI0SCS0N_TM64P1OUT12_GP16_MDIOD_TM64P1IN12" pad="D17"/>
<connect gate="D" pin="SPI0SCS1N_TM64P0OUT12_GP17_MDIOCLK_TM64P0IN12" pad="E16"/>
<connect gate="D" pin="SPI0SCS2N_UART0RTS_GP81_MIIRXD0_SATACPDET" pad="D16"/>
<connect gate="D" pin="SPI0SCS3N_UART0CTS_GP82_MIIRXD1_SATAMPSWITCH" pad="E17"/>
<connect gate="D" pin="SPI0SCS4N_UART0TXD_GP83_MIIRXD2" pad="D18"/>
<connect gate="D" pin="SPI0SCS5N_UART0RXD_GP84_MIIRXD3" pad="C19"/>
<connect gate="D" pin="SPI0SIMO_EPWMSYNC0_GP85_MIICRS" pad="C18"/>
<connect gate="D" pin="SPI0SOMI_EPWMSYNCI_GP86_MIIRXER" pad="C16"/>
<connect gate="D" pin="SPI1CLK_GP213" pad="G19"/>
<connect gate="D" pin="SPI1ENAN_GP212" pad="H16"/>
<connect gate="D" pin="SPI1SCS0N_EPWM1B_GP214_TM64P3IN12" pad="E19"/>
<connect gate="D" pin="SPI1SCS1N_EPWM1A_GP215_TM64P2IN12" pad="F18"/>
<connect gate="D" pin="SPI1SCS2N_UART1TXD_SATACPPOD_GP10" pad="F19"/>
<connect gate="D" pin="SPI1SCS3N_UART1RXD_SATALED_GP11" pad="E18"/>
<connect gate="D" pin="SPI1SCS4N_UART2TXD_I2C1SDA_GP12" pad="F16"/>
<connect gate="D" pin="SPI1SCS5N_UART2RXD_I2C1SCL_GP13" pad="F17"/>
<connect gate="D" pin="SPI1SCS6N_I2C0SDA_TM64P3OUT12_GP14" pad="G18"/>
<connect gate="D" pin="SPI1SCS7N_I2C0SCL_TM64P2OUT12_GP15" pad="G16"/>
<connect gate="D" pin="SPI1SIMO_GP210" pad="G17"/>
<connect gate="D" pin="SPI1SOMI_GP211" pad="H17"/>
<connect gate="D" pin="TCK" pad="J15"/>
<connect gate="D" pin="TDI" pad="M16"/>
<connect gate="D" pin="TDO" pad="J18"/>
<connect gate="D" pin="TMS" pad="L16"/>
<connect gate="D" pin="TRSTN" pad="L17"/>
<connect gate="D" pin="UHPIHCNTL0_UPPCHACLOCK_GP611" pad="U17"/>
<connect gate="D" pin="UHPIHCNTL1_UPPCHASTART_GP610" pad="W15"/>
<connect gate="D" pin="UHPIHHWIL_UPPCHAENABLE_GP69" pad="U16"/>
<connect gate="D" pin="UHPIHINTN_GP612" pad="R16"/>
<connect gate="D" pin="UHPIHRDYN_GP613" pad="R17"/>
<connect gate="D" pin="UHPIHRWN_UPPCHAWAIT_GP68" pad="T15"/>
<connect gate="D" pin="UPPCHBWAIT_GP812" pad="G3"/>
<connect gate="D" pin="USB0DRVVBUS" pad="K18"/>
<connect gate="E" pin="VPIFCLKIN0_UHPIHCSN_GP67_UPP2XTXCLK" pad="W14"/>
<connect gate="E" pin="VPIFCLKIN1_UHPIHDS1N_GP66" pad="V15"/>
<connect gate="E" pin="VPIFCLKIN2_MMCSD1DAT3_GP64" pad="H3"/>
<connect gate="E" pin="VPIFCLKIN3_MMCSD1DAT1_GP62" pad="J3"/>
<connect gate="E" pin="VPIFCLKO2_MMCSD1DAT2_GP63" pad="K3"/>
<connect gate="E" pin="VPIFCLKO3_GP61" pad="K4"/>
<connect gate="E" pin="VPIFDIN0_UHPIHD8_UPPD8_RMIICRSDV" pad="W19"/>
<connect gate="E" pin="VPIFDIN10_UHPIHD2_UPPD2" pad="R19"/>
<connect gate="E" pin="VPIFDIN11_UHPIHD3_UPPD3" pad="R18"/>
<connect gate="E" pin="VPIFDIN12_UHPIHD4_UPPD4" pad="T16"/>
<connect gate="E" pin="VPIFDIN13FIELD_UHPIHD5_UPPD5" pad="U19"/>
<connect gate="E" pin="VPIFDIN14HSYNC_UHPIHD6_UPPD6" pad="V19"/>
<connect gate="E" pin="VPIFDIN15VSYNC_UHPIHD7_UPPD7" pad="V18"/>
<connect gate="E" pin="VPIFDIN1_UHPIHD9_UPPD9_RMIIMHZ50CLK" pad="W18"/>
<connect gate="E" pin="VPIFDIN2_UHPIHD10_UPPD10_RMIIRXER" pad="W17"/>
<connect gate="E" pin="VPIFDIN3_UHPIHD11_UPPD11_RMIIRXD0" pad="V17"/>
<connect gate="E" pin="VPIFDIN4_UHPIHD12_UPPD12_RMIIRXD1" pad="W16"/>
<connect gate="E" pin="VPIFDIN5_UHPIHD13_UPPD13_RMIITXEN" pad="R14"/>
<connect gate="E" pin="VPIFDIN6_UHPIHD14_UPPD14_RMIITXD0" pad="V16"/>
<connect gate="E" pin="VPIFDIN7_UHPIHD15_UPPD15_RMIITXD1" pad="U18"/>
<connect gate="E" pin="VPIFDIN8_UHPIHD0_UPPD0_GP65" pad="P17"/>
<connect gate="E" pin="VPIFDIN9_UHPIHD1_UPPD1" pad="R15"/>
<connect gate="E" pin="VPIFDOUT0_LCDD0_UPPXD8_GP78" pad="W1"/>
<connect gate="E" pin="VPIFDOUT10_LCDD10_UPPXD2_GP72_BOOT2" pad="T2"/>
<connect gate="E" pin="VPIFDOUT11_LCDD11_UPPXD3_GP73_BOOT3" pad="T3"/>
<connect gate="E" pin="VPIFDOUT12_LCDD12_UPPXD4_GP74_BOOT4" pad="R1"/>
<connect gate="E" pin="VPIFDOUT13_LCDD13_UPPXD5_GP75_BOOT5" pad="R2"/>
<connect gate="E" pin="VPIFDOUT14_LCDD14_UPPXD6_GP76_BOOT6" pad="R3"/>
<connect gate="E" pin="VPIFDOUT15_LCDD15_UPPXD7_GP77_BOOT7" pad="P4"/>
<connect gate="E" pin="VPIFDOUT1_LCDD1_UPPXD9_GP79" pad="W2"/>
<connect gate="E" pin="VPIFDOUT2_LCDD2_UPPXD10_GP710" pad="W3"/>
<connect gate="E" pin="VPIFDOUT3_LCDD3_UPPXD11_GP711" pad="V1"/>
<connect gate="E" pin="VPIFDOUT4_LCDD4_UPPXD12_GP712" pad="V2"/>
<connect gate="E" pin="VPIFDOUT5_LCDD5_UPPXD13_GP713" pad="V3"/>
<connect gate="E" pin="VPIFDOUT6_LCDD6_UPPXD14_GP714" pad="U1"/>
<connect gate="E" pin="VPIFDOUT7_LCDD7_UPPXD15_GP715" pad="U2"/>
<connect gate="E" pin="VPIFDOUT8_LCDD8_UPPXD0_GP70_BOOT0" pad="U3"/>
<connect gate="E" pin="VPIFDOUT9_LCDD9_UPPXD1_GP71_BOOT1" pad="T1"/>
<connect gate="P" pin="VDD@1" pad="E15"/>
<connect gate="P" pin="VDD@10" pad="H7"/>
<connect gate="P" pin="VDD@11" pad="J12"/>
<connect gate="P" pin="VDD@12" pad="J6"/>
<connect gate="P" pin="VDD@13" pad="K12"/>
<connect gate="P" pin="VDD@14" pad="K6"/>
<connect gate="P" pin="VDD@15" pad="L12"/>
<connect gate="P" pin="VDD@16" pad="M8"/>
<connect gate="P" pin="VDD@17" pad="M9"/>
<connect gate="P" pin="VDD@18" pad="N8"/>
<connect gate="P" pin="VDD@19" pad="F14"/>
<connect gate="P" pin="VDD@2" pad="G13"/>
<connect gate="P" pin="VDD@20" pad="G10"/>
<connect gate="P" pin="VDD@21" pad="G11"/>
<connect gate="P" pin="VDD@22" pad="G12"/>
<connect gate="P" pin="VDD@23" pad="G6"/>
<connect gate="P" pin="VDD@24" pad="J13"/>
<connect gate="P" pin="VDD@25" pad="K5"/>
<connect gate="P" pin="VDD@26" pad="L6"/>
<connect gate="P" pin="VDD@27" pad="P13"/>
<connect gate="P" pin="VDD@28" pad="R13"/>
<connect gate="P" pin="VDD@29" pad="L14"/>
<connect gate="P" pin="VDD@3" pad="G7"/>
<connect gate="P" pin="VDD@30" pad="N4"/>
<connect gate="P" pin="VDD@31" pad="M12"/>
<connect gate="P" pin="VDD@32" pad="L15"/>
<connect gate="P" pin="VDD@33" pad="N15"/>
<connect gate="P" pin="VDD@34" pad="N17"/>
<connect gate="P" pin="VDD@35" pad="P14"/>
<connect gate="P" pin="VDD@36" pad="N14"/>
<connect gate="P" pin="VDD@37" pad="N18"/>
<connect gate="P" pin="VDD@38" pad="P15"/>
<connect gate="P" pin="VDD@39" pad="H14"/>
<connect gate="P" pin="VDD@4" pad="G8"/>
<connect gate="P" pin="VDD@40" pad="R6"/>
<connect gate="P" pin="VDD@41" pad="E5"/>
<connect gate="P" pin="VDD@42" pad="N7"/>
<connect gate="P" pin="VDD@43" pad="P3"/>
<connect gate="P" pin="VDD@44" pad="N10"/>
<connect gate="P" pin="VDD@45" pad="N6"/>
<connect gate="P" pin="VDD@46" pad="N9"/>
<connect gate="P" pin="VDD@47" pad="P10"/>
<connect gate="P" pin="VDD@48" pad="P7"/>
<connect gate="P" pin="VDD@49" pad="P8"/>
<connect gate="P" pin="VDD@5" pad="H10"/>
<connect gate="P" pin="VDD@50" pad="P9"/>
<connect gate="P" pin="VDD@51" pad="R7"/>
<connect gate="P" pin="VDD@52" pad="R8"/>
<connect gate="P" pin="VDD@53" pad="R9"/>
<connect gate="P" pin="VDD@54" pad="E14"/>
<connect gate="P" pin="VDD@55" pad="F10"/>
<connect gate="P" pin="VDD@56" pad="F11"/>
<connect gate="P" pin="VDD@57" pad="F12"/>
<connect gate="P" pin="VDD@58" pad="F13"/>
<connect gate="P" pin="VDD@59" pad="F6"/>
<connect gate="P" pin="VDD@6" pad="H11"/>
<connect gate="P" pin="VDD@60" pad="F7"/>
<connect gate="P" pin="VDD@61" pad="F8"/>
<connect gate="P" pin="VDD@62" pad="G9"/>
<connect gate="P" pin="VDD@63" pad="F5"/>
<connect gate="P" pin="VDD@64" pad="G5"/>
<connect gate="P" pin="VDD@65" pad="H5"/>
<connect gate="P" pin="VDD@66" pad="J5"/>
<connect gate="P" pin="VDD@67" pad="L4"/>
<connect gate="P" pin="VDD@68" pad="P5"/>
<connect gate="P" pin="VDD@69" pad="P6"/>
<connect gate="P" pin="VDD@7" pad="H12"/>
<connect gate="P" pin="VDD@70" pad="R4"/>
<connect gate="P" pin="VDD@71" pad="K13"/>
<connect gate="P" pin="VDD@72" pad="L13"/>
<connect gate="P" pin="VDD@73" pad="M13"/>
<connect gate="P" pin="VDD@74" pad="N13"/>
<connect gate="P" pin="VDD@75" pad="P12"/>
<connect gate="P" pin="VDD@76" pad="J14"/>
<connect gate="P" pin="VDD@77" pad="K15"/>
<connect gate="P" pin="VDD@78" pad="F15"/>
<connect gate="P" pin="VDD@79" pad="G14"/>
<connect gate="P" pin="VDD@8" pad="H13"/>
<connect gate="P" pin="VDD@80" pad="G15"/>
<connect gate="P" pin="VDD@81" pad="M2"/>
<connect gate="P" pin="VDD@82" pad="P1"/>
<connect gate="P" pin="VDD@83" pad="P2"/>
<connect gate="P" pin="VDD@84" pad="T19"/>
<connect gate="P" pin="VDD@9" pad="H6"/>
<connect gate="P" pin="VSS@1" pad="A19"/>
<connect gate="P" pin="VSS@10" pad="K10"/>
<connect gate="P" pin="VSS@11" pad="K11"/>
<connect gate="P" pin="VSS@12" pad="K7"/>
<connect gate="P" pin="VSS@13" pad="K8"/>
<connect gate="P" pin="VSS@14" pad="K9"/>
<connect gate="P" pin="VSS@15" pad="L10"/>
<connect gate="P" pin="VSS@16" pad="L11"/>
<connect gate="P" pin="VSS@17" pad="L5"/>
<connect gate="P" pin="VSS@18" pad="L7"/>
<connect gate="P" pin="VSS@19" pad="L8"/>
<connect gate="P" pin="VSS@2" pad="H15"/>
<connect gate="P" pin="VSS@20" pad="L9"/>
<connect gate="P" pin="VSS@21" pad="M10"/>
<connect gate="P" pin="VSS@22" pad="M11"/>
<connect gate="P" pin="VSS@23" pad="M4"/>
<connect gate="P" pin="VSS@24" pad="M5"/>
<connect gate="P" pin="VSS@25" pad="M6"/>
<connect gate="P" pin="VSS@26" pad="M7"/>
<connect gate="P" pin="VSS@27" pad="N11"/>
<connect gate="P" pin="VSS@28" pad="N12"/>
<connect gate="P" pin="VSS@29" pad="N5"/>
<connect gate="P" pin="VSS@3" pad="H8"/>
<connect gate="P" pin="VSS@30" pad="P11"/>
<connect gate="P" pin="VSS@31" pad="M17"/>
<connect gate="P" pin="VSS@32" pad="M15"/>
<connect gate="P" pin="VSS@33" pad="N16"/>
<connect gate="P" pin="VSS@34" pad="M14"/>
<connect gate="P" pin="VSS@35" pad="H1"/>
<connect gate="P" pin="VSS@36" pad="H2"/>
<connect gate="P" pin="VSS@37" pad="K1"/>
<connect gate="P" pin="VSS@38" pad="K2"/>
<connect gate="P" pin="VSS@39" pad="L3"/>
<connect gate="P" pin="VSS@4" pad="H9"/>
<connect gate="P" pin="VSS@40" pad="M1"/>
<connect gate="P" pin="VSS@41" pad="L18"/>
<connect gate="P" pin="VSS@42" pad="H18"/>
<connect gate="P" pin="VSS@5" pad="J10"/>
<connect gate="P" pin="VSS@6" pad="J11"/>
<connect gate="P" pin="VSS@7" pad="J7"/>
<connect gate="P" pin="VSS@8" pad="J8"/>
<connect gate="P" pin="VSS@9" pad="J9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OMAP-L138ZCE" prefix="IC">
<description>&lt;b&gt;OMAP-L138 Low-Power Applications Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Source: sprm377a.bsm&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/omap-l138.pdf&lt;br&gt;&lt;i&gt;Connect-List generated from &lt;/i&gt;&lt;b&gt;OMAPL138ZCE.DEV&lt;/b&gt; Variant &lt;b&gt;''&lt;/b&gt; with &lt;i&gt;&lt;b&gt;connect-device-split-symbol-03.ulp&lt;/b&gt;&lt;/i&gt;</description>
<gates>
<gate name="A" symbol="OMAP-L138_ZCE-A"/>
<gate name="B" symbol="OMAP-L138_ZCE-B"/>
<gate name="C" symbol="OMAP-L138_ZCE-C"/>
<gate name="D" symbol="OMAP-L138_ZCE-D"/>
<gate name="E" symbol="OMAP-L138_ZCE-E"/>
<gate name="P" symbol="OMAP-L138_ZCE-P"/>
</gates>
<devices>
<device name="" package="ZCE_S-PBGA-N361">
<connects>
<connect gate="A" pin="ACLKR_GP015" pad="A1"/>
<connect gate="A" pin="ACLKX_GP014" pad="B1"/>
<connect gate="A" pin="AFSR0_GP013" pad="C2"/>
<connect gate="A" pin="AFSX0_GP012" pad="B2"/>
<connect gate="A" pin="AHCLKR_UART1RTS_GP011" pad="A2"/>
<connect gate="A" pin="AHCLKX_USBREFCLKIN_UART1CTS_GP010" pad="A3"/>
<connect gate="A" pin="AMUTEIN_RTCALARM_UART2CTS_GP08_DEEPSLEEPN" pad="F4"/>
<connect gate="A" pin="AMUTE_UART2RTS_GP09" pad="D5"/>
<connect gate="A" pin="AXR00_ECAP0APWM0_GP87_MIITXD0_CLKS0" pad="F3"/>
<connect gate="A" pin="AXR010_DR1_GP02" pad="D4"/>
<connect gate="A" pin="AXR011_FSX1_GP03" pad="C5"/>
<connect gate="A" pin="AXR012_FSR1_GP04" pad="C4"/>
<connect gate="A" pin="AXR013_CLKX1_GP05" pad="B3"/>
<connect gate="A" pin="AXR014_CLKR1_GP06" pad="B4"/>
<connect gate="A" pin="AXR015_EPWM0TZ0_ECAP2APWM2_GP07" pad="A4"/>
<connect gate="A" pin="AXR01_DX0_GP19MIITXD1" pad="E1"/>
<connect gate="A" pin="AXR02_DR0_GP110_MIITXD2" pad="E2"/>
<connect gate="A" pin="AXR03_FSX0_GP111_MIITXD3" pad="E3"/>
<connect gate="A" pin="AXR04_FSR0_GP112_MIICOL" pad="D1"/>
<connect gate="A" pin="AXR05_CLKX0_GP113_MIITXCLK" pad="D3"/>
<connect gate="A" pin="AXR06_CLKR0_GP114_MIITXEN" pad="C1"/>
<connect gate="A" pin="AXR07_EPWM1TZ0_GP115" pad="D2"/>
<connect gate="A" pin="AXR08_CLKS1_ECAP1APWM1_GP00" pad="E4"/>
<connect gate="A" pin="AXR09_DX1_GP01" pad="C3"/>
<connect gate="A" pin="CLKOUT_UHPIHDS2N_GP614" pad="T18"/>
<connect gate="B" pin="DDRA0" pad="U7"/>
<connect gate="B" pin="DDRA1" pad="T7"/>
<connect gate="B" pin="DDRA10" pad="W4"/>
<connect gate="B" pin="DDRA11" pad="T4"/>
<connect gate="B" pin="DDRA12" pad="V4"/>
<connect gate="B" pin="DDRA13" pad="T5"/>
<connect gate="B" pin="DDRA2" pad="W6"/>
<connect gate="B" pin="DDRA3" pad="V6"/>
<connect gate="B" pin="DDRA4" pad="U5"/>
<connect gate="B" pin="DDRA5" pad="V5"/>
<connect gate="B" pin="DDRA6" pad="W5"/>
<connect gate="B" pin="DDRA7" pad="U6"/>
<connect gate="B" pin="DDRA8" pad="U4"/>
<connect gate="B" pin="DDRA9" pad="T6"/>
<connect gate="B" pin="DDRBA0" pad="V8"/>
<connect gate="B" pin="DDRBA1" pad="T9"/>
<connect gate="B" pin="DDRBA2" pad="U8"/>
<connect gate="B" pin="DDRCASN" pad="U9"/>
<connect gate="B" pin="DDRCKE" pad="V7"/>
<connect gate="B" pin="DDRCLKN" pad="W7"/>
<connect gate="B" pin="DDRCLKP" pad="W8"/>
<connect gate="B" pin="DDRCSN" pad="V9"/>
<connect gate="B" pin="DDRD0" pad="U15"/>
<connect gate="B" pin="DDRD1" pad="U14"/>
<connect gate="B" pin="DDRD10" pad="T10"/>
<connect gate="B" pin="DDRD11" pad="T12"/>
<connect gate="B" pin="DDRD12" pad="U10"/>
<connect gate="B" pin="DDRD13" pad="V10"/>
<connect gate="B" pin="DDRD14" pad="U11"/>
<connect gate="B" pin="DDRD15" pad="W10"/>
<connect gate="B" pin="DDRD2" pad="V14"/>
<connect gate="B" pin="DDRD3" pad="U13"/>
<connect gate="B" pin="DDRD4" pad="V13"/>
<connect gate="B" pin="DDRD5" pad="V12"/>
<connect gate="B" pin="DDRD6" pad="W12"/>
<connect gate="B" pin="DDRD7" pad="W11"/>
<connect gate="B" pin="DDRD8" pad="T13"/>
<connect gate="B" pin="DDRD9" pad="T11"/>
<connect gate="B" pin="DDRDQGATE0" pad="R11"/>
<connect gate="B" pin="DDRDQGATE1" pad="R12"/>
<connect gate="B" pin="DDRDQM0N" pad="W13"/>
<connect gate="B" pin="DDRDQM1N" pad="R10"/>
<connect gate="B" pin="DDRDQS0" pad="T14"/>
<connect gate="B" pin="DDRDQS1" pad="V11"/>
<connect gate="B" pin="DDRRASN" pad="W9"/>
<connect gate="B" pin="DDRWEN" pad="T8"/>
<connect gate="C" pin="EMAA0_GP50" pad="C14"/>
<connect gate="C" pin="EMAA10_GP510" pad="C12"/>
<connect gate="C" pin="EMAA11_GP511" pad="B12"/>
<connect gate="C" pin="EMAA12_GP512" pad="D13"/>
<connect gate="C" pin="EMAA13_GP513" pad="D11"/>
<connect gate="C" pin="EMAA14_MMCSD0DAT7_GP514" pad="A12"/>
<connect gate="C" pin="EMAA15_MMCSD0DAT6_GP515" pad="C11"/>
<connect gate="C" pin="EMAA16_MMCSD0DAT5_GP40" pad="E12"/>
<connect gate="C" pin="EMAA17_MMCSD0DAT4_GP41" pad="B11"/>
<connect gate="C" pin="EMAA18_MMCSD0DAT3_GP42" pad="E11"/>
<connect gate="C" pin="EMAA19_MMCSD0DAT2_GP43" pad="C10"/>
<connect gate="C" pin="EMAA1_GP51" pad="D15"/>
<connect gate="C" pin="EMAA20_MMCSD0DAT1_GP44" pad="A11"/>
<connect gate="C" pin="EMAA21_MMCSD0DAT0_GP45" pad="B10"/>
<connect gate="C" pin="EMAA22_MMCSD0CMD_GP46" pad="A10"/>
<connect gate="C" pin="EMAA23_MMCSD0CLK_GP47" pad="E9"/>
<connect gate="C" pin="EMAA2_GP52" pad="B14"/>
<connect gate="C" pin="EMAA3_GP53" pad="D14"/>
<connect gate="C" pin="EMAA4_GP54" pad="A14"/>
<connect gate="C" pin="EMAA5_GP55" pad="C13"/>
<connect gate="C" pin="EMAA6_GP56" pad="E13"/>
<connect gate="C" pin="EMAA7_GP57" pad="B13"/>
<connect gate="C" pin="EMAA8_GP58" pad="A13"/>
<connect gate="C" pin="EMAA9_GP59" pad="D12"/>
<connect gate="C" pin="EMABA0_GP28" pad="C15"/>
<connect gate="C" pin="EMABA1_GP29" pad="A15"/>
<connect gate="C" pin="EMACASN_GP24" pad="A9"/>
<connect gate="C" pin="EMACLK_GP27" pad="B7"/>
<connect gate="C" pin="EMACS0N_GP20" pad="A18"/>
<connect gate="C" pin="EMACS2N_GP315" pad="B17"/>
<connect gate="C" pin="EMACS3N_GP314" pad="A17"/>
<connect gate="C" pin="EMACS4N_GP313" pad="F9"/>
<connect gate="C" pin="EMACS5N_GP212" pad="B16"/>
<connect gate="C" pin="EMAD0_GP48" pad="C9"/>
<connect gate="C" pin="EMAD10_GP32" pad="A7"/>
<connect gate="C" pin="EMAD11_GP33" pad="D6"/>
<connect gate="C" pin="EMAD12_GP34" pad="A6"/>
<connect gate="C" pin="EMAD13_GP35" pad="B6"/>
<connect gate="C" pin="EMAD14_GP36" pad="C7"/>
<connect gate="C" pin="EMAD15_GP37" pad="E6"/>
<connect gate="C" pin="EMAD1_GP49" pad="A8"/>
<connect gate="C" pin="EMAD2_GP410" pad="B8"/>
<connect gate="C" pin="EMAD3_GP411" pad="E8"/>
<connect gate="C" pin="EMAD4_GP412" pad="B5"/>
<connect gate="C" pin="EMAD5_GP413" pad="E7"/>
<connect gate="C" pin="EMAD6_GP414" pad="C6"/>
<connect gate="C" pin="EMAD7_GP415" pad="D7"/>
<connect gate="C" pin="EMAD8_GP30" pad="E10"/>
<connect gate="C" pin="EMAD9_GP31" pad="D9"/>
<connect gate="C" pin="EMAOEN_GP310" pad="B15"/>
<connect gate="C" pin="EMARASN_GP25" pad="A16"/>
<connect gate="C" pin="EMARNW_GP39" pad="D10"/>
<connect gate="C" pin="EMASDCKE_GP26" pad="D8"/>
<connect gate="C" pin="EMAWAIT0_GP38" pad="B18"/>
<connect gate="C" pin="EMAWAIT1_GP21" pad="B19"/>
<connect gate="C" pin="EMAWEDQM0N_GP23" pad="C8"/>
<connect gate="C" pin="EMAWEDQM1N_GP22" pad="A5"/>
<connect gate="C" pin="EMAWEN_GP311" pad="B9"/>
<connect gate="C" pin="EMU0" pad="J16"/>
<connect gate="C" pin="EMU1" pad="K16"/>
<connect gate="D" pin="LCDACENBCSN_GP60" pad="R5"/>
<connect gate="D" pin="MMCSD1CLK_UPPCHBSTART_GP814" pad="G2"/>
<connect gate="D" pin="MMCSD1CMD_UPPCHBENABLE_GP813" pad="J4"/>
<connect gate="D" pin="MMCSD1DAT0_UPPCHBCLOCK_GP815" pad="G1"/>
<connect gate="D" pin="MMCSD1DAT4_LCDVSYNC_GP88" pad="G4"/>
<connect gate="D" pin="MMCSD1DAT5_LCDHSYNC_GP89" pad="H4"/>
<connect gate="D" pin="MMCSD1DAT6_LCDMCLK_GP810" pad="F2"/>
<connect gate="D" pin="MMCSD1DAT7_LCDPCLK_GP811" pad="F1"/>
<connect gate="D" pin="NMIN" pad="J17"/>
<connect gate="D" pin="RESETN" pad="K14"/>
<connect gate="D" pin="RESETOUTN_UHPIHASN_GP615" pad="T17"/>
<connect gate="D" pin="SATARXN" pad="L2"/>
<connect gate="D" pin="SATARXP" pad="L1"/>
<connect gate="D" pin="SATATXP" pad="J1"/>
<connect gate="D" pin="SPI0CLK_EPWM0A_GP18_MIIRXCLK" pad="D19"/>
<connect gate="D" pin="SPI0ENAN_EPWM0B_MIIRXDV" pad="C17"/>
<connect gate="D" pin="SPI0SCS0N_TM64P1OUT12_GP16_MDIOD_TM64P1IN12" pad="D17"/>
<connect gate="D" pin="SPI0SCS1N_TM64P0OUT12_GP17_MDIOCLK_TM64P0IN12" pad="E16"/>
<connect gate="D" pin="SPI0SCS2N_UART0RTS_GP81_MIIRXD0_SATACPDET" pad="D16"/>
<connect gate="D" pin="SPI0SCS3N_UART0CTS_GP82_MIIRXD1_SATAMPSWITCH" pad="E17"/>
<connect gate="D" pin="SPI0SCS4N_UART0TXD_GP83_MIIRXD2" pad="D18"/>
<connect gate="D" pin="SPI0SCS5N_UART0RXD_GP84_MIIRXD3" pad="C19"/>
<connect gate="D" pin="SPI0SIMO_EPWMSYNC0_GP85_MIICRS" pad="C18"/>
<connect gate="D" pin="SPI0SOMI_EPWMSYNCI_GP86_MIIRXER" pad="C16"/>
<connect gate="D" pin="SPI1CLK_GP213" pad="G19"/>
<connect gate="D" pin="SPI1ENAN_GP212" pad="H16"/>
<connect gate="D" pin="SPI1SCS0N_EPWM1B_GP214_TM64P3IN12" pad="E19"/>
<connect gate="D" pin="SPI1SCS1N_EPWM1A_GP215_TM64P2IN12" pad="F18"/>
<connect gate="D" pin="SPI1SCS2N_UART1TXD_SATACPPOD_GP10" pad="F19"/>
<connect gate="D" pin="SPI1SCS3N_UART1RXD_SATALED_GP11" pad="E18"/>
<connect gate="D" pin="SPI1SCS4N_UART2TXD_I2C1SDA_GP12" pad="F16"/>
<connect gate="D" pin="SPI1SCS5N_UART2RXD_I2C1SCL_GP13" pad="F17"/>
<connect gate="D" pin="SPI1SCS6N_I2C0SDA_TM64P3OUT12_GP14" pad="G18"/>
<connect gate="D" pin="SPI1SCS7N_I2C0SCL_TM64P2OUT12_GP15" pad="G16"/>
<connect gate="D" pin="SPI1SIMO_GP210" pad="G17"/>
<connect gate="D" pin="SPI1SOMI_GP211" pad="H17"/>
<connect gate="D" pin="TCK" pad="J15"/>
<connect gate="D" pin="TDI" pad="M16"/>
<connect gate="D" pin="TDO" pad="J18"/>
<connect gate="D" pin="TMS" pad="L16"/>
<connect gate="D" pin="TRSTN" pad="L17"/>
<connect gate="D" pin="UHPIHCNTL0_UPPCHACLOCK_GP611" pad="U17"/>
<connect gate="D" pin="UHPIHCNTL1_UPPCHASTART_GP610" pad="W15"/>
<connect gate="D" pin="UHPIHHWIL_UPPCHAENABLE_GP69" pad="U16"/>
<connect gate="D" pin="UHPIHINTN_GP612" pad="R16"/>
<connect gate="D" pin="UHPIHRDYN_GP613" pad="R17"/>
<connect gate="D" pin="UHPIHRWN_UPPCHAWAIT_GP68" pad="T15"/>
<connect gate="D" pin="UPPCHBWAIT_GP812" pad="G3"/>
<connect gate="D" pin="USB0DRVVBUS" pad="K18"/>
<connect gate="E" pin="VPIFCLKIN0_UHPIHCSN_GP67_UPP2XTXCLK" pad="W14"/>
<connect gate="E" pin="VPIFCLKIN1_UHPIHDS1N_GP66" pad="V15"/>
<connect gate="E" pin="VPIFCLKIN2_MMCSD1DAT3_GP64" pad="H3"/>
<connect gate="E" pin="VPIFCLKIN3_MMCSD1DAT1_GP62" pad="J3"/>
<connect gate="E" pin="VPIFCLKO2_MMCSD1DAT2_GP63" pad="K3"/>
<connect gate="E" pin="VPIFCLKO3_GP61" pad="K4"/>
<connect gate="E" pin="VPIFDIN0_UHPIHD8_UPPD8_RMIICRSDV" pad="W19"/>
<connect gate="E" pin="VPIFDIN10_UHPIHD2_UPPD2" pad="R19"/>
<connect gate="E" pin="VPIFDIN11_UHPIHD3_UPPD3" pad="R18"/>
<connect gate="E" pin="VPIFDIN12_UHPIHD4_UPPD4" pad="T16"/>
<connect gate="E" pin="VPIFDIN13FIELD_UHPIHD5_UPPD5" pad="U19"/>
<connect gate="E" pin="VPIFDIN14HSYNC_UHPIHD6_UPPD6" pad="V19"/>
<connect gate="E" pin="VPIFDIN15VSYNC_UHPIHD7_UPPD7" pad="V18"/>
<connect gate="E" pin="VPIFDIN1_UHPIHD9_UPPD9_RMIIMHZ50CLK" pad="W18"/>
<connect gate="E" pin="VPIFDIN2_UHPIHD10_UPPD10_RMIIRXER" pad="W17"/>
<connect gate="E" pin="VPIFDIN3_UHPIHD11_UPPD11_RMIIRXD0" pad="V17"/>
<connect gate="E" pin="VPIFDIN4_UHPIHD12_UPPD12_RMIIRXD1" pad="W16"/>
<connect gate="E" pin="VPIFDIN5_UHPIHD13_UPPD13_RMIITXEN" pad="R14"/>
<connect gate="E" pin="VPIFDIN6_UHPIHD14_UPPD14_RMIITXD0" pad="V16"/>
<connect gate="E" pin="VPIFDIN7_UHPIHD15_UPPD15_RMIITXD1" pad="U18"/>
<connect gate="E" pin="VPIFDIN8_UHPIHD0_UPPD0_GP65" pad="P17"/>
<connect gate="E" pin="VPIFDIN9_UHPIHD1_UPPD1" pad="R15"/>
<connect gate="E" pin="VPIFDOUT0_LCDD0_UPPXD8_GP78" pad="W1"/>
<connect gate="E" pin="VPIFDOUT10_LCDD10_UPPXD2_GP72_BOOT2" pad="T2"/>
<connect gate="E" pin="VPIFDOUT11_LCDD11_UPPXD3_GP73_BOOT3" pad="T3"/>
<connect gate="E" pin="VPIFDOUT12_LCDD12_UPPXD4_GP74_BOOT4" pad="R1"/>
<connect gate="E" pin="VPIFDOUT13_LCDD13_UPPXD5_GP75_BOOT5" pad="R2"/>
<connect gate="E" pin="VPIFDOUT14_LCDD14_UPPXD6_GP76_BOOT6" pad="R3"/>
<connect gate="E" pin="VPIFDOUT15_LCDD15_UPPXD7_GP77_BOOT7" pad="P4"/>
<connect gate="E" pin="VPIFDOUT1_LCDD1_UPPXD9_GP79" pad="W2"/>
<connect gate="E" pin="VPIFDOUT2_LCDD2_UPPXD10_GP710" pad="W3"/>
<connect gate="E" pin="VPIFDOUT3_LCDD3_UPPXD11_GP711" pad="V1"/>
<connect gate="E" pin="VPIFDOUT4_LCDD4_UPPXD12_GP712" pad="V2"/>
<connect gate="E" pin="VPIFDOUT5_LCDD5_UPPXD13_GP713" pad="V3"/>
<connect gate="E" pin="VPIFDOUT6_LCDD6_UPPXD14_GP714" pad="U1"/>
<connect gate="E" pin="VPIFDOUT7_LCDD7_UPPXD15_GP715" pad="U2"/>
<connect gate="E" pin="VPIFDOUT8_LCDD8_UPPXD0_GP70_BOOT0" pad="U3"/>
<connect gate="E" pin="VPIFDOUT9_LCDD9_UPPXD1_GP71_BOOT1" pad="T1"/>
<connect gate="P" pin="VDD@1" pad="E15"/>
<connect gate="P" pin="VDD@10" pad="H7"/>
<connect gate="P" pin="VDD@11" pad="J12"/>
<connect gate="P" pin="VDD@12" pad="J6"/>
<connect gate="P" pin="VDD@13" pad="K12"/>
<connect gate="P" pin="VDD@14" pad="K6"/>
<connect gate="P" pin="VDD@15" pad="L12"/>
<connect gate="P" pin="VDD@16" pad="M8"/>
<connect gate="P" pin="VDD@17" pad="M9"/>
<connect gate="P" pin="VDD@18" pad="N8"/>
<connect gate="P" pin="VDD@19" pad="F14"/>
<connect gate="P" pin="VDD@2" pad="G13"/>
<connect gate="P" pin="VDD@20" pad="G10"/>
<connect gate="P" pin="VDD@21" pad="G11"/>
<connect gate="P" pin="VDD@22" pad="G12"/>
<connect gate="P" pin="VDD@23" pad="G6"/>
<connect gate="P" pin="VDD@24" pad="J13"/>
<connect gate="P" pin="VDD@25" pad="K5"/>
<connect gate="P" pin="VDD@26" pad="L6"/>
<connect gate="P" pin="VDD@27" pad="P13"/>
<connect gate="P" pin="VDD@28" pad="R13"/>
<connect gate="P" pin="VDD@29" pad="L14"/>
<connect gate="P" pin="VDD@3" pad="G7"/>
<connect gate="P" pin="VDD@30" pad="N4"/>
<connect gate="P" pin="VDD@31" pad="M12"/>
<connect gate="P" pin="VDD@32" pad="L15"/>
<connect gate="P" pin="VDD@33" pad="N15"/>
<connect gate="P" pin="VDD@34" pad="N17"/>
<connect gate="P" pin="VDD@35" pad="P14"/>
<connect gate="P" pin="VDD@36" pad="N14"/>
<connect gate="P" pin="VDD@37" pad="N18"/>
<connect gate="P" pin="VDD@38" pad="P15"/>
<connect gate="P" pin="VDD@39" pad="H14"/>
<connect gate="P" pin="VDD@4" pad="G8"/>
<connect gate="P" pin="VDD@40" pad="R6"/>
<connect gate="P" pin="VDD@41" pad="E5"/>
<connect gate="P" pin="VDD@42" pad="N7"/>
<connect gate="P" pin="VDD@43" pad="P3"/>
<connect gate="P" pin="VDD@44" pad="N10"/>
<connect gate="P" pin="VDD@45" pad="N6"/>
<connect gate="P" pin="VDD@46" pad="N9"/>
<connect gate="P" pin="VDD@47" pad="P10"/>
<connect gate="P" pin="VDD@48" pad="P7"/>
<connect gate="P" pin="VDD@49" pad="P8"/>
<connect gate="P" pin="VDD@5" pad="H10"/>
<connect gate="P" pin="VDD@50" pad="P9"/>
<connect gate="P" pin="VDD@51" pad="R7"/>
<connect gate="P" pin="VDD@52" pad="R8"/>
<connect gate="P" pin="VDD@53" pad="R9"/>
<connect gate="P" pin="VDD@54" pad="E14"/>
<connect gate="P" pin="VDD@55" pad="F10"/>
<connect gate="P" pin="VDD@56" pad="F11"/>
<connect gate="P" pin="VDD@57" pad="F12"/>
<connect gate="P" pin="VDD@58" pad="F13"/>
<connect gate="P" pin="VDD@59" pad="F6"/>
<connect gate="P" pin="VDD@6" pad="H11"/>
<connect gate="P" pin="VDD@60" pad="F7"/>
<connect gate="P" pin="VDD@61" pad="F8"/>
<connect gate="P" pin="VDD@62" pad="G9"/>
<connect gate="P" pin="VDD@63" pad="F5"/>
<connect gate="P" pin="VDD@64" pad="G5"/>
<connect gate="P" pin="VDD@65" pad="H5"/>
<connect gate="P" pin="VDD@66" pad="J5"/>
<connect gate="P" pin="VDD@67" pad="L4"/>
<connect gate="P" pin="VDD@68" pad="P5"/>
<connect gate="P" pin="VDD@69" pad="P6"/>
<connect gate="P" pin="VDD@7" pad="H12"/>
<connect gate="P" pin="VDD@70" pad="R4"/>
<connect gate="P" pin="VDD@71" pad="K13"/>
<connect gate="P" pin="VDD@72" pad="L13"/>
<connect gate="P" pin="VDD@73" pad="M13"/>
<connect gate="P" pin="VDD@74" pad="N13"/>
<connect gate="P" pin="VDD@75" pad="P12"/>
<connect gate="P" pin="VDD@76" pad="J14"/>
<connect gate="P" pin="VDD@77" pad="K15"/>
<connect gate="P" pin="VDD@78" pad="F15"/>
<connect gate="P" pin="VDD@79" pad="G14"/>
<connect gate="P" pin="VDD@8" pad="H13"/>
<connect gate="P" pin="VDD@80" pad="G15"/>
<connect gate="P" pin="VDD@81" pad="M2"/>
<connect gate="P" pin="VDD@82" pad="P1"/>
<connect gate="P" pin="VDD@83" pad="P2"/>
<connect gate="P" pin="VDD@84" pad="T19"/>
<connect gate="P" pin="VDD@9" pad="H6"/>
<connect gate="P" pin="VSS@1" pad="A19"/>
<connect gate="P" pin="VSS@10" pad="K10"/>
<connect gate="P" pin="VSS@11" pad="K11"/>
<connect gate="P" pin="VSS@12" pad="K7"/>
<connect gate="P" pin="VSS@13" pad="K8"/>
<connect gate="P" pin="VSS@14" pad="K9"/>
<connect gate="P" pin="VSS@15" pad="L10"/>
<connect gate="P" pin="VSS@16" pad="L11"/>
<connect gate="P" pin="VSS@17" pad="L5"/>
<connect gate="P" pin="VSS@18" pad="L7"/>
<connect gate="P" pin="VSS@19" pad="L8"/>
<connect gate="P" pin="VSS@2" pad="H15"/>
<connect gate="P" pin="VSS@20" pad="L9"/>
<connect gate="P" pin="VSS@21" pad="M10"/>
<connect gate="P" pin="VSS@22" pad="M11"/>
<connect gate="P" pin="VSS@23" pad="M4"/>
<connect gate="P" pin="VSS@24" pad="M5"/>
<connect gate="P" pin="VSS@25" pad="M6"/>
<connect gate="P" pin="VSS@26" pad="M7"/>
<connect gate="P" pin="VSS@27" pad="N11"/>
<connect gate="P" pin="VSS@28" pad="N12"/>
<connect gate="P" pin="VSS@29" pad="N5"/>
<connect gate="P" pin="VSS@3" pad="H8"/>
<connect gate="P" pin="VSS@30" pad="P11"/>
<connect gate="P" pin="VSS@31" pad="M17"/>
<connect gate="P" pin="VSS@32" pad="M15"/>
<connect gate="P" pin="VSS@33" pad="N16"/>
<connect gate="P" pin="VSS@34" pad="M14"/>
<connect gate="P" pin="VSS@35" pad="H1"/>
<connect gate="P" pin="VSS@36" pad="H2"/>
<connect gate="P" pin="VSS@37" pad="K1"/>
<connect gate="P" pin="VSS@38" pad="K2"/>
<connect gate="P" pin="VSS@39" pad="L3"/>
<connect gate="P" pin="VSS@4" pad="H9"/>
<connect gate="P" pin="VSS@40" pad="M1"/>
<connect gate="P" pin="VSS@41" pad="L18"/>
<connect gate="P" pin="VSS@42" pad="H18"/>
<connect gate="P" pin="VSS@5" pad="J10"/>
<connect gate="P" pin="VSS@6" pad="J11"/>
<connect gate="P" pin="VSS@7" pad="J7"/>
<connect gate="P" pin="VSS@8" pad="J8"/>
<connect gate="P" pin="VSS@9" pad="J9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320VC5509A" prefix="IC">
<description>&lt;b&gt;TMS320VC5509A Fixed-Point Digital Signal Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Source: sprm155a.bsm&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/tms320vc5509a.pdf</description>
<gates>
<gate name="G$1" symbol="TMS320VC5509A"/>
</gates>
<devices>
<device name="" package="GHH_S-PBGA-N179">
<connects>
<connect gate="G$1" pin="A0" pad="L7"/>
<connect gate="G$1" pin="A0E" pad="H11"/>
<connect gate="G$1" pin="A1" pad="M7"/>
<connect gate="G$1" pin="A10" pad="N4"/>
<connect gate="G$1" pin="A11" pad="L4"/>
<connect gate="G$1" pin="A12" pad="P3"/>
<connect gate="G$1" pin="A13" pad="N3"/>
<connect gate="G$1" pin="A14" pad="K9"/>
<connect gate="G$1" pin="A15" pad="M8"/>
<connect gate="G$1" pin="A16" pad="P7"/>
<connect gate="G$1" pin="A17" pad="P5"/>
<connect gate="G$1" pin="A18" pad="K1"/>
<connect gate="G$1" pin="A19" pad="H3"/>
<connect gate="G$1" pin="A2" pad="K7"/>
<connect gate="G$1" pin="A20" pad="G3"/>
<connect gate="G$1" pin="A3" pad="K6"/>
<connect gate="G$1" pin="A4" pad="P6"/>
<connect gate="G$1" pin="A5" pad="M6"/>
<connect gate="G$1" pin="A6" pad="L6"/>
<connect gate="G$1" pin="A7" pad="N5"/>
<connect gate="G$1" pin="A8" pad="L5"/>
<connect gate="G$1" pin="A9" pad="P4"/>
<connect gate="G$1" pin="ADVDD" pad="F10"/>
<connect gate="G$1" pin="ADVSS" pad="E12"/>
<connect gate="G$1" pin="AIN0" pad="D14"/>
<connect gate="G$1" pin="AIN1" pad="D13"/>
<connect gate="G$1" pin="AIN2" pad="D12"/>
<connect gate="G$1" pin="AIN3" pad="E11"/>
<connect gate="G$1" pin="AVDD" pad="C14"/>
<connect gate="G$1" pin="AVSS@1" pad="B14"/>
<connect gate="G$1" pin="AVSS@2" pad="C13"/>
<connect gate="G$1" pin="C0" pad="G5"/>
<connect gate="G$1" pin="C1" pad="G2"/>
<connect gate="G$1" pin="C10" pad="M1"/>
<connect gate="G$1" pin="C11" pad="K3"/>
<connect gate="G$1" pin="C12" pad="L3"/>
<connect gate="G$1" pin="C13" pad="M2"/>
<connect gate="G$1" pin="C14" pad="L2"/>
<connect gate="G$1" pin="C2" pad="G4"/>
<connect gate="G$1" pin="C3" pad="H1"/>
<connect gate="G$1" pin="C4" pad="H4"/>
<connect gate="G$1" pin="C5" pad="H5"/>
<connect gate="G$1" pin="C6" pad="J1"/>
<connect gate="G$1" pin="C7" pad="J3"/>
<connect gate="G$1" pin="C8" pad="J4"/>
<connect gate="G$1" pin="C9" pad="K2"/>
<connect gate="G$1" pin="CLKOUT" pad="F5"/>
<connect gate="G$1" pin="CLKR0" pad="B5"/>
<connect gate="G$1" pin="CLKX0" pad="C6"/>
<connect gate="G$1" pin="CVDD@1" pad="A6"/>
<connect gate="G$1" pin="CVDD@10" pad="M4"/>
<connect gate="G$1" pin="CVDD@11" pad="M11"/>
<connect gate="G$1" pin="CVDD@12" pad="N8"/>
<connect gate="G$1" pin="CVDD@2" pad="B2"/>
<connect gate="G$1" pin="CVDD@3" pad="B7"/>
<connect gate="G$1" pin="CVDD@4" pad="B8"/>
<connect gate="G$1" pin="CVDD@5" pad="C10"/>
<connect gate="G$1" pin="CVDD@6" pad="G1"/>
<connect gate="G$1" pin="CVDD@7" pad="J5"/>
<connect gate="G$1" pin="CVDD@8" pad="J11"/>
<connect gate="G$1" pin="CVDD@9" pad="L14"/>
<connect gate="G$1" pin="D0" pad="L8"/>
<connect gate="G$1" pin="D1" pad="K8"/>
<connect gate="G$1" pin="D10" pad="P12"/>
<connect gate="G$1" pin="D11" pad="N12"/>
<connect gate="G$1" pin="D12" pad="M14"/>
<connect gate="G$1" pin="D13" pad="L11"/>
<connect gate="G$1" pin="D14" pad="L12"/>
<connect gate="G$1" pin="D15" pad="L13"/>
<connect gate="G$1" pin="D2" pad="P9"/>
<connect gate="G$1" pin="D3" pad="M9"/>
<connect gate="G$1" pin="D4" pad="L9"/>
<connect gate="G$1" pin="D5" pad="P10"/>
<connect gate="G$1" pin="D6" pad="M10"/>
<connect gate="G$1" pin="D7" pad="P11"/>
<connect gate="G$1" pin="D8" pad="N11"/>
<connect gate="G$1" pin="D9" pad="L10"/>
<connect gate="G$1" pin="DN" pad="D3"/>
<connect gate="G$1" pin="DP" pad="D4"/>
<connect gate="G$1" pin="DR0" pad="D6"/>
<connect gate="G$1" pin="DVDD@1" pad="A4"/>
<connect gate="G$1" pin="DVDD@10" pad="K10"/>
<connect gate="G$1" pin="DVDD@11" pad="M12"/>
<connect gate="G$1" pin="DVDD@12" pad="N6"/>
<connect gate="G$1" pin="DVDD@13" pad="N13"/>
<connect gate="G$1" pin="DVDD@14" pad="P8"/>
<connect gate="G$1" pin="DVDD@15" pad="P13"/>
<connect gate="G$1" pin="DVDD@16" pad="P14"/>
<connect gate="G$1" pin="DVDD@2" pad="A8"/>
<connect gate="G$1" pin="DVDD@3" pad="D9"/>
<connect gate="G$1" pin="DVDD@4" pad="E3"/>
<connect gate="G$1" pin="DVDD@5" pad="E6"/>
<connect gate="G$1" pin="DVDD@6" pad="F13"/>
<connect gate="G$1" pin="DVDD@7" pad="H2"/>
<connect gate="G$1" pin="DVDD@8" pad="H10"/>
<connect gate="G$1" pin="DVDD@9" pad="J2"/>
<connect gate="G$1" pin="DX0" pad="E7"/>
<connect gate="G$1" pin="EMU0" pad="K11"/>
<connect gate="G$1" pin="EMU1" pad="K12"/>
<connect gate="G$1" pin="FSR0" pad="A5"/>
<connect gate="G$1" pin="FSX0" pad="B6"/>
<connect gate="G$1" pin="GPIO0" pad="F3"/>
<connect gate="G$1" pin="GPIO1" pad="E1"/>
<connect gate="G$1" pin="GPIO2" pad="E2"/>
<connect gate="G$1" pin="GPIO3" pad="B3"/>
<connect gate="G$1" pin="GPIO4" pad="A3"/>
<connect gate="G$1" pin="GPIO5" pad="D5"/>
<connect gate="G$1" pin="GPIO6" pad="C4"/>
<connect gate="G$1" pin="GPIO7" pad="D1"/>
<connect gate="G$1" pin="NC1" pad="C3"/>
<connect gate="G$1" pin="NC2" pad="E10"/>
<connect gate="G$1" pin="NINT0" pad="G14"/>
<connect gate="G$1" pin="NINT1" pad="G13"/>
<connect gate="G$1" pin="NINT2" pad="G10"/>
<connect gate="G$1" pin="NINT3" pad="F14"/>
<connect gate="G$1" pin="NINT4" pad="F12"/>
<connect gate="G$1" pin="NRESET" pad="H12"/>
<connect gate="G$1" pin="PU" pad="C1"/>
<connect gate="G$1" pin="RCVDD" pad="C12"/>
<connect gate="G$1" pin="RDVDD@1" pad="A13"/>
<connect gate="G$1" pin="RDVDD@2" pad="A14"/>
<connect gate="G$1" pin="RDVDD@3" pad="B13"/>
<connect gate="G$1" pin="RTCINX1" pad="A12"/>
<connect gate="G$1" pin="RTCINX2" pad="B12"/>
<connect gate="G$1" pin="RVDD@1" pad="J10"/>
<connect gate="G$1" pin="RVDD@2" pad="L1"/>
<connect gate="G$1" pin="RVDD@3" pad="N7"/>
<connect gate="G$1" pin="S10" pad="D7"/>
<connect gate="G$1" pin="S11" pad="D8"/>
<connect gate="G$1" pin="S12" pad="A7"/>
<connect gate="G$1" pin="S13" pad="E9"/>
<connect gate="G$1" pin="S14" pad="C8"/>
<connect gate="G$1" pin="S15" pad="E8"/>
<connect gate="G$1" pin="S20" pad="A9"/>
<connect gate="G$1" pin="S21" pad="A10"/>
<connect gate="G$1" pin="S22" pad="C9"/>
<connect gate="G$1" pin="S23" pad="A11"/>
<connect gate="G$1" pin="S24" pad="B10"/>
<connect gate="G$1" pin="S25" pad="D10"/>
<connect gate="G$1" pin="SCL" pad="H14"/>
<connect gate="G$1" pin="SDA" pad="H13"/>
<connect gate="G$1" pin="TCK" pad="J13"/>
<connect gate="G$1" pin="TDI" pad="K14"/>
<connect gate="G$1" pin="TDO" pad="K13"/>
<connect gate="G$1" pin="TINOUT0" pad="B4"/>
<connect gate="G$1" pin="TMS" pad="J14"/>
<connect gate="G$1" pin="TRST" pad="J12"/>
<connect gate="G$1" pin="USBPLLVDD" pad="G11"/>
<connect gate="G$1" pin="USBPLLVSS" pad="G12"/>
<connect gate="G$1" pin="USBVDD" pad="D2"/>
<connect gate="G$1" pin="VSS@1" pad="A2"/>
<connect gate="G$1" pin="VSS@10" pad="E4"/>
<connect gate="G$1" pin="VSS@11" pad="E5"/>
<connect gate="G$1" pin="VSS@12" pad="E13"/>
<connect gate="G$1" pin="VSS@13" pad="F4"/>
<connect gate="G$1" pin="VSS@14" pad="F11"/>
<connect gate="G$1" pin="VSS@15" pad="K4"/>
<connect gate="G$1" pin="VSS@16" pad="K5"/>
<connect gate="G$1" pin="VSS@17" pad="M3"/>
<connect gate="G$1" pin="VSS@18" pad="M5"/>
<connect gate="G$1" pin="VSS@19" pad="M13"/>
<connect gate="G$1" pin="VSS@2" pad="B1"/>
<connect gate="G$1" pin="VSS@20" pad="N1"/>
<connect gate="G$1" pin="VSS@21" pad="N2"/>
<connect gate="G$1" pin="VSS@22" pad="N9"/>
<connect gate="G$1" pin="VSS@23" pad="N10"/>
<connect gate="G$1" pin="VSS@24" pad="N14"/>
<connect gate="G$1" pin="VSS@25" pad="P1"/>
<connect gate="G$1" pin="VSS@26" pad="P2"/>
<connect gate="G$1" pin="VSS@3" pad="B9"/>
<connect gate="G$1" pin="VSS@4" pad="B11"/>
<connect gate="G$1" pin="VSS@5" pad="C2"/>
<connect gate="G$1" pin="VSS@6" pad="C5"/>
<connect gate="G$1" pin="VSS@7" pad="C7"/>
<connect gate="G$1" pin="VSS@8" pad="C11"/>
<connect gate="G$1" pin="VSS@9" pad="D11"/>
<connect gate="G$1" pin="X1" pad="F1"/>
<connect gate="G$1" pin="X2CLKIN" pad="F2"/>
<connect gate="G$1" pin="XF" pad="E14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TMS320VC5509AGHHR"/>
<attribute name="OC_FARNELL" value="1610194"/>
<attribute name="OC_NEWARK" value="92H7535"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320VC5509" prefix="IC">
<description>&lt;b&gt;TMS320VC5509A Fixed-Point Digital Signal Processor&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Source: sprm155a.bsm&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/tms320vc5509a.pdf&lt;br&gt;&lt;i&gt;Connect-List generated from &lt;/i&gt;&lt;b&gt;TMS320VC5509A.DEV&lt;/b&gt; Variant &lt;b&gt;''&lt;/b&gt; with &lt;i&gt;&lt;b&gt;connect-device-split-symbol.ulp&lt;/b&gt;&lt;/i&gt;</description>
<gates>
<gate name="A" symbol="TMS320VC5509-A"/>
<gate name="B" symbol="TMS320VC5509-B"/>
<gate name="D" symbol="TMS320VC5509-D"/>
<gate name="E" symbol="TMS320VC5509-E"/>
<gate name="C" symbol="TMS320VC5509-C"/>
<gate name="F" symbol="TMS320VC5509-P"/>
</gates>
<devices>
<device name="" package="GHH_S-PBGA-N179">
<connects>
<connect gate="A" pin="A0" pad="L7"/>
<connect gate="A" pin="A0E" pad="H11"/>
<connect gate="A" pin="A1" pad="M7"/>
<connect gate="A" pin="A10" pad="N4"/>
<connect gate="A" pin="A11" pad="L4"/>
<connect gate="A" pin="A12" pad="P3"/>
<connect gate="A" pin="A13" pad="N3"/>
<connect gate="A" pin="A14" pad="K9"/>
<connect gate="A" pin="A15" pad="M8"/>
<connect gate="A" pin="A16" pad="P7"/>
<connect gate="A" pin="A17" pad="P5"/>
<connect gate="A" pin="A18" pad="K1"/>
<connect gate="A" pin="A19" pad="H3"/>
<connect gate="A" pin="A2" pad="K7"/>
<connect gate="A" pin="A20" pad="G3"/>
<connect gate="A" pin="A3" pad="K6"/>
<connect gate="A" pin="A4" pad="P6"/>
<connect gate="A" pin="A5" pad="M6"/>
<connect gate="A" pin="A6" pad="L6"/>
<connect gate="A" pin="A7" pad="N5"/>
<connect gate="A" pin="A8" pad="L5"/>
<connect gate="A" pin="A9" pad="P4"/>
<connect gate="B" pin="C0" pad="G5"/>
<connect gate="B" pin="C1" pad="G2"/>
<connect gate="B" pin="C10" pad="M1"/>
<connect gate="B" pin="C11" pad="K3"/>
<connect gate="B" pin="C12" pad="L3"/>
<connect gate="B" pin="C13" pad="M2"/>
<connect gate="B" pin="C14" pad="L2"/>
<connect gate="B" pin="C2" pad="G4"/>
<connect gate="B" pin="C3" pad="H1"/>
<connect gate="B" pin="C4" pad="H4"/>
<connect gate="B" pin="C5" pad="H5"/>
<connect gate="B" pin="C6" pad="J1"/>
<connect gate="B" pin="C7" pad="J3"/>
<connect gate="B" pin="C8" pad="J4"/>
<connect gate="B" pin="C9" pad="K2"/>
<connect gate="B" pin="CLKOUT" pad="F5"/>
<connect gate="B" pin="CLKR0" pad="B5"/>
<connect gate="B" pin="CLKX0" pad="C6"/>
<connect gate="C" pin="D0" pad="L8"/>
<connect gate="C" pin="D1" pad="K8"/>
<connect gate="C" pin="D10" pad="P12"/>
<connect gate="C" pin="D11" pad="N12"/>
<connect gate="C" pin="D12" pad="M14"/>
<connect gate="C" pin="D13" pad="L11"/>
<connect gate="C" pin="D14" pad="L12"/>
<connect gate="C" pin="D15" pad="L13"/>
<connect gate="C" pin="D2" pad="P9"/>
<connect gate="C" pin="D3" pad="M9"/>
<connect gate="C" pin="D4" pad="L9"/>
<connect gate="C" pin="D5" pad="P10"/>
<connect gate="C" pin="D6" pad="M10"/>
<connect gate="C" pin="D7" pad="P11"/>
<connect gate="C" pin="D8" pad="N11"/>
<connect gate="C" pin="D9" pad="L10"/>
<connect gate="C" pin="DN" pad="D3"/>
<connect gate="C" pin="DP" pad="D4"/>
<connect gate="C" pin="DR0" pad="D6"/>
<connect gate="D" pin="ADVDD" pad="F10"/>
<connect gate="D" pin="ADVSS" pad="E12"/>
<connect gate="D" pin="AIN0" pad="D14"/>
<connect gate="D" pin="AIN1" pad="D13"/>
<connect gate="D" pin="AIN2" pad="D12"/>
<connect gate="D" pin="AIN3" pad="E11"/>
<connect gate="D" pin="AVDD" pad="C14"/>
<connect gate="D" pin="AVSS@1" pad="B14"/>
<connect gate="D" pin="AVSS@2" pad="C13"/>
<connect gate="D" pin="DX0" pad="E7"/>
<connect gate="D" pin="EMU0" pad="K11"/>
<connect gate="D" pin="EMU1" pad="K12"/>
<connect gate="D" pin="FSR0" pad="A5"/>
<connect gate="D" pin="FSX0" pad="B6"/>
<connect gate="D" pin="GPIO0" pad="F3"/>
<connect gate="D" pin="GPIO1" pad="E1"/>
<connect gate="D" pin="GPIO2" pad="E2"/>
<connect gate="D" pin="GPIO3" pad="B3"/>
<connect gate="D" pin="GPIO4" pad="A3"/>
<connect gate="D" pin="GPIO5" pad="D5"/>
<connect gate="D" pin="GPIO6" pad="C4"/>
<connect gate="D" pin="GPIO7" pad="D1"/>
<connect gate="D" pin="NC1" pad="C3"/>
<connect gate="D" pin="NC2" pad="E10"/>
<connect gate="D" pin="NINT0" pad="G14"/>
<connect gate="D" pin="NINT1" pad="G13"/>
<connect gate="D" pin="NINT2" pad="G10"/>
<connect gate="D" pin="NINT3" pad="F14"/>
<connect gate="D" pin="NINT4" pad="F12"/>
<connect gate="D" pin="NRESET" pad="H12"/>
<connect gate="D" pin="PU" pad="C1"/>
<connect gate="D" pin="RTCINX1" pad="A12"/>
<connect gate="D" pin="RTCINX2" pad="B12"/>
<connect gate="E" pin="S10" pad="D7"/>
<connect gate="E" pin="S11" pad="D8"/>
<connect gate="E" pin="S12" pad="A7"/>
<connect gate="E" pin="S13" pad="E9"/>
<connect gate="E" pin="S14" pad="C8"/>
<connect gate="E" pin="S15" pad="E8"/>
<connect gate="E" pin="S20" pad="A9"/>
<connect gate="E" pin="S21" pad="A10"/>
<connect gate="E" pin="S22" pad="C9"/>
<connect gate="E" pin="S23" pad="A11"/>
<connect gate="E" pin="S24" pad="B10"/>
<connect gate="E" pin="S25" pad="D10"/>
<connect gate="E" pin="SCL" pad="H14"/>
<connect gate="E" pin="SDA" pad="H13"/>
<connect gate="E" pin="TCK" pad="J13"/>
<connect gate="E" pin="TDI" pad="K14"/>
<connect gate="E" pin="TDO" pad="K13"/>
<connect gate="E" pin="TINOUT0" pad="B4"/>
<connect gate="E" pin="TMS" pad="J14"/>
<connect gate="E" pin="TRST" pad="J12"/>
<connect gate="E" pin="USBPLLVDD" pad="G11"/>
<connect gate="E" pin="USBPLLVSS" pad="G12"/>
<connect gate="E" pin="USBVDD" pad="D2"/>
<connect gate="E" pin="X1" pad="F1"/>
<connect gate="E" pin="X2CLKIN" pad="F2"/>
<connect gate="E" pin="XF" pad="E14"/>
<connect gate="F" pin="CVDD@1" pad="A6"/>
<connect gate="F" pin="CVDD@10" pad="M4"/>
<connect gate="F" pin="CVDD@11" pad="M11"/>
<connect gate="F" pin="CVDD@12" pad="N8"/>
<connect gate="F" pin="CVDD@2" pad="B2"/>
<connect gate="F" pin="CVDD@3" pad="B7"/>
<connect gate="F" pin="CVDD@4" pad="B8"/>
<connect gate="F" pin="CVDD@5" pad="C10"/>
<connect gate="F" pin="CVDD@6" pad="G1"/>
<connect gate="F" pin="CVDD@7" pad="J5"/>
<connect gate="F" pin="CVDD@8" pad="J11"/>
<connect gate="F" pin="CVDD@9" pad="L14"/>
<connect gate="F" pin="DVDD@1" pad="A4"/>
<connect gate="F" pin="DVDD@10" pad="K10"/>
<connect gate="F" pin="DVDD@11" pad="M12"/>
<connect gate="F" pin="DVDD@12" pad="N6"/>
<connect gate="F" pin="DVDD@13" pad="N13"/>
<connect gate="F" pin="DVDD@14" pad="P8"/>
<connect gate="F" pin="DVDD@15" pad="P13"/>
<connect gate="F" pin="DVDD@16" pad="P14"/>
<connect gate="F" pin="DVDD@2" pad="A8"/>
<connect gate="F" pin="DVDD@3" pad="D9"/>
<connect gate="F" pin="DVDD@4" pad="E3"/>
<connect gate="F" pin="DVDD@5" pad="E6"/>
<connect gate="F" pin="DVDD@6" pad="F13"/>
<connect gate="F" pin="DVDD@7" pad="H2"/>
<connect gate="F" pin="DVDD@8" pad="H10"/>
<connect gate="F" pin="DVDD@9" pad="J2"/>
<connect gate="F" pin="RCVDD" pad="C12"/>
<connect gate="F" pin="RDVDD@1" pad="A13"/>
<connect gate="F" pin="RDVDD@2" pad="A14"/>
<connect gate="F" pin="RDVDD@3" pad="B13"/>
<connect gate="F" pin="RVDD@1" pad="J10"/>
<connect gate="F" pin="RVDD@2" pad="L1"/>
<connect gate="F" pin="RVDD@3" pad="N7"/>
<connect gate="F" pin="VSS@1" pad="A2"/>
<connect gate="F" pin="VSS@10" pad="E4"/>
<connect gate="F" pin="VSS@11" pad="E5"/>
<connect gate="F" pin="VSS@12" pad="E13"/>
<connect gate="F" pin="VSS@13" pad="F4"/>
<connect gate="F" pin="VSS@14" pad="F11"/>
<connect gate="F" pin="VSS@15" pad="K4"/>
<connect gate="F" pin="VSS@16" pad="K5"/>
<connect gate="F" pin="VSS@17" pad="M3"/>
<connect gate="F" pin="VSS@18" pad="M5"/>
<connect gate="F" pin="VSS@19" pad="M13"/>
<connect gate="F" pin="VSS@2" pad="B1"/>
<connect gate="F" pin="VSS@20" pad="N1"/>
<connect gate="F" pin="VSS@21" pad="N2"/>
<connect gate="F" pin="VSS@22" pad="N9"/>
<connect gate="F" pin="VSS@23" pad="N10"/>
<connect gate="F" pin="VSS@24" pad="N14"/>
<connect gate="F" pin="VSS@25" pad="P1"/>
<connect gate="F" pin="VSS@26" pad="P2"/>
<connect gate="F" pin="VSS@3" pad="B9"/>
<connect gate="F" pin="VSS@4" pad="B11"/>
<connect gate="F" pin="VSS@5" pad="C2"/>
<connect gate="F" pin="VSS@6" pad="C5"/>
<connect gate="F" pin="VSS@7" pad="C7"/>
<connect gate="F" pin="VSS@8" pad="C11"/>
<connect gate="F" pin="VSS@9" pad="D11"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TMS320VC5509AGHH"/>
<attribute name="OC_FARNELL" value="1610194"/>
<attribute name="OC_NEWARK" value="14N9600"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TUSB2046B" prefix="IC">
<description>&lt;b&gt;4-PORT HUB FOR THE UNIVERSAL SERIAL BUS WITH OPTIONAL SERIAL EEPROM INTERFACE&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 30&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/tusb2046b.pdf</description>
<gates>
<gate name="G$1" symbol="TUSB2046B"/>
</gates>
<devices>
<device name="VFR" package="VF_S-PQFP-G32">
<connects>
<connect gate="G$1" pin="!EXTMEM" pad="26"/>
<connect gate="G$1" pin="!OVRCUR1" pad="10"/>
<connect gate="G$1" pin="!OVRCUR2" pad="14"/>
<connect gate="G$1" pin="!OVRCUR3" pad="18"/>
<connect gate="G$1" pin="!OVRCUR4" pad="22"/>
<connect gate="G$1" pin="!PWRON1" pad="9"/>
<connect gate="G$1" pin="!PWRON2" pad="13"/>
<connect gate="G$1" pin="!PWRON3" pad="17"/>
<connect gate="G$1" pin="!PWRON4" pad="21"/>
<connect gate="G$1" pin="!RESET" pad="4"/>
<connect gate="G$1" pin="BUSPWR" pad="8"/>
<connect gate="G$1" pin="DM0" pad="2"/>
<connect gate="G$1" pin="DM1" pad="11"/>
<connect gate="G$1" pin="DM2" pad="15"/>
<connect gate="G$1" pin="DM3" pad="19"/>
<connect gate="G$1" pin="DM4" pad="23"/>
<connect gate="G$1" pin="DP0" pad="1"/>
<connect gate="G$1" pin="DP1" pad="12"/>
<connect gate="G$1" pin="DP2" pad="16"/>
<connect gate="G$1" pin="DP3" pad="20"/>
<connect gate="G$1" pin="DP4" pad="24"/>
<connect gate="G$1" pin="EECLK" pad="5"/>
<connect gate="G$1" pin="EEDATA/GANGED" pad="6"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="SUSPND" pad="32"/>
<connect gate="G$1" pin="TSTMODE" pad="31"/>
<connect gate="G$1" pin="TSTPLL/48MCLK" pad="27"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VCC@1" pad="25"/>
<connect gate="G$1" pin="XTAL1" pad="30"/>
<connect gate="G$1" pin="XTAL2" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="TUSB2046BVFR"/>
<attribute name="OC_FARNELL" value="1470507"/>
<attribute name="OC_NEWARK" value="77C1806"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TUSB2046BIRHB" prefix="IC">
<description>&lt;b&gt;4-PORT HUB FOR THE UNIVERSAL SERIAL BUS WITH OPTIONAL SERIAL EEPROM INTERFACE&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tusb2046b.pdf</description>
<gates>
<gate name="G$1" symbol="TUSB2046B"/>
<gate name="EXP" symbol="EXP10"/>
</gates>
<devices>
<device name="IRHB" package="RHB_S-PQFP-N32">
<connects>
<connect gate="EXP" pin="EXP" pad="EXP"/>
<connect gate="EXP" pin="EXP@1" pad="EXP@1"/>
<connect gate="EXP" pin="EXP@2" pad="EXP@2"/>
<connect gate="EXP" pin="EXP@3" pad="EXP@3"/>
<connect gate="EXP" pin="EXP@4" pad="EXP@4"/>
<connect gate="EXP" pin="EXP@5" pad="EXP@5"/>
<connect gate="EXP" pin="EXP@6" pad="EXP@6"/>
<connect gate="EXP" pin="EXP@7" pad="EXP@7"/>
<connect gate="EXP" pin="EXP@8" pad="EXP@8"/>
<connect gate="EXP" pin="EXP@9" pad="EXP@9"/>
<connect gate="G$1" pin="!EXTMEM" pad="26"/>
<connect gate="G$1" pin="!OVRCUR1" pad="10"/>
<connect gate="G$1" pin="!OVRCUR2" pad="14"/>
<connect gate="G$1" pin="!OVRCUR3" pad="18"/>
<connect gate="G$1" pin="!OVRCUR4" pad="22"/>
<connect gate="G$1" pin="!PWRON1" pad="9"/>
<connect gate="G$1" pin="!PWRON2" pad="13"/>
<connect gate="G$1" pin="!PWRON3" pad="17"/>
<connect gate="G$1" pin="!PWRON4" pad="21"/>
<connect gate="G$1" pin="!RESET" pad="4"/>
<connect gate="G$1" pin="BUSPWR" pad="8"/>
<connect gate="G$1" pin="DM0" pad="2"/>
<connect gate="G$1" pin="DM1" pad="11"/>
<connect gate="G$1" pin="DM2" pad="15"/>
<connect gate="G$1" pin="DM3" pad="19"/>
<connect gate="G$1" pin="DM4" pad="23"/>
<connect gate="G$1" pin="DP0" pad="1"/>
<connect gate="G$1" pin="DP1" pad="12"/>
<connect gate="G$1" pin="DP2" pad="16"/>
<connect gate="G$1" pin="DP3" pad="20"/>
<connect gate="G$1" pin="DP4" pad="24"/>
<connect gate="G$1" pin="EECLK" pad="5"/>
<connect gate="G$1" pin="EEDATA/GANGED" pad="6"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="GND@1" pad="28"/>
<connect gate="G$1" pin="SUSPND" pad="32"/>
<connect gate="G$1" pin="TSTMODE" pad="31"/>
<connect gate="G$1" pin="TSTPLL/48MCLK" pad="27"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VCC@1" pad="25"/>
<connect gate="G$1" pin="XTAL1" pad="30"/>
<connect gate="G$1" pin="XTAL2" pad="29"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TUSB2046BIRHBT"/>
<attribute name="OC_FARNELL" value="1610201"/>
<attribute name="OC_NEWARK" value="14N8499"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVCR162245A" prefix="IC">
<description>&lt;b&gt;16-BIT BUS TRANSCEIVER WITH 3-STATE OUTPUTS&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 33&lt;/i&gt;&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvcr162245.pdf</description>
<gates>
<gate name="G$1" symbol="SN74LVCR162245A"/>
</gates>
<devices>
<device name="" package="DL_R-PDSO-G48">
<connects>
<connect gate="G$1" pin="1!OE" pad="48"/>
<connect gate="G$1" pin="1A1" pad="47"/>
<connect gate="G$1" pin="1A2" pad="46"/>
<connect gate="G$1" pin="1A3" pad="44"/>
<connect gate="G$1" pin="1A4" pad="43"/>
<connect gate="G$1" pin="1A5" pad="41"/>
<connect gate="G$1" pin="1A6" pad="40"/>
<connect gate="G$1" pin="1A7" pad="38"/>
<connect gate="G$1" pin="1A8" pad="37"/>
<connect gate="G$1" pin="1B1" pad="2"/>
<connect gate="G$1" pin="1B2" pad="3"/>
<connect gate="G$1" pin="1B3" pad="5"/>
<connect gate="G$1" pin="1B4" pad="6"/>
<connect gate="G$1" pin="1B5" pad="8"/>
<connect gate="G$1" pin="1B6" pad="9"/>
<connect gate="G$1" pin="1B7" pad="11"/>
<connect gate="G$1" pin="1B8" pad="12"/>
<connect gate="G$1" pin="1DIR" pad="1"/>
<connect gate="G$1" pin="2!OE" pad="25"/>
<connect gate="G$1" pin="2A1" pad="36"/>
<connect gate="G$1" pin="2A2" pad="35"/>
<connect gate="G$1" pin="2A3" pad="33"/>
<connect gate="G$1" pin="2A4" pad="32"/>
<connect gate="G$1" pin="2A5" pad="30"/>
<connect gate="G$1" pin="2A6" pad="29"/>
<connect gate="G$1" pin="2A7" pad="27"/>
<connect gate="G$1" pin="2A8" pad="26"/>
<connect gate="G$1" pin="2B1" pad="13"/>
<connect gate="G$1" pin="2B2" pad="14"/>
<connect gate="G$1" pin="2B3" pad="16"/>
<connect gate="G$1" pin="2B4" pad="17"/>
<connect gate="G$1" pin="2B5" pad="19"/>
<connect gate="G$1" pin="2B6" pad="20"/>
<connect gate="G$1" pin="2B7" pad="22"/>
<connect gate="G$1" pin="2B8" pad="23"/>
<connect gate="G$1" pin="2DIR" pad="24"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="15"/>
<connect gate="G$1" pin="GND@3" pad="21"/>
<connect gate="G$1" pin="GND@4" pad="28"/>
<connect gate="G$1" pin="GND@5" pad="34"/>
<connect gate="G$1" pin="GND@6" pad="39"/>
<connect gate="G$1" pin="GND@7" pad="45"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VCC@1" pad="18"/>
<connect gate="G$1" pin="VCC@2" pad="31"/>
<connect gate="G$1" pin="VCC@3" pad="42"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SN74LVCR162245DL"/>
<attribute name="OC_FARNELL" value="1739707"/>
<attribute name="OC_NEWARK" value="50R6613"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430F23" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/msp430f2471.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430F23X"/>
</gates>
<devices>
<device name="TRGC" package="RGC_S-PVQFV-N64">
<connects>
<connect gate="G$1" pin="!RST!/NMI" pad="58"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="AVSS" pad="62"/>
<connect gate="G$1" pin="DVCC" pad="1"/>
<connect gate="G$1" pin="DVSS" pad="63"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="P1_0/TACLK/CAOUT" pad="12"/>
<connect gate="G$1" pin="P1_1/TA0" pad="13"/>
<connect gate="G$1" pin="P1_2/TA1" pad="14"/>
<connect gate="G$1" pin="P1_3/TA2" pad="15"/>
<connect gate="G$1" pin="P1_4/SMCLK" pad="16"/>
<connect gate="G$1" pin="P1_5/TA0" pad="17"/>
<connect gate="G$1" pin="P1_6/TA1" pad="18"/>
<connect gate="G$1" pin="P1_7/TA2" pad="19"/>
<connect gate="G$1" pin="P2_0/ACLK/CA2" pad="20"/>
<connect gate="G$1" pin="P2_1/TAINCLK/CA3" pad="21"/>
<connect gate="G$1" pin="P2_2/CAOUT/TA0/CA4" pad="22"/>
<connect gate="G$1" pin="P2_3/CA0/TA1" pad="23"/>
<connect gate="G$1" pin="P2_4/CA1/TA2" pad="24"/>
<connect gate="G$1" pin="P2_5/ROSC/CA5" pad="25"/>
<connect gate="G$1" pin="P2_6/ADC12CLK/CA6" pad="26"/>
<connect gate="G$1" pin="P2_7/TA0/CA7" pad="27"/>
<connect gate="G$1" pin="P3_0/UCB0STE/UCA0CLK" pad="28"/>
<connect gate="G$1" pin="P3_1/UCB0SIMO/UCB0SDA" pad="29"/>
<connect gate="G$1" pin="P3_2/UCB0SOMI/UCB0SCL" pad="30"/>
<connect gate="G$1" pin="P3_3/UCB0CLK/UCA0STE" pad="31"/>
<connect gate="G$1" pin="P3_4/UCA0TXD/UCA0SIMO" pad="32"/>
<connect gate="G$1" pin="P3_5/UCA0RXD/UCA0SOMI" pad="33"/>
<connect gate="G$1" pin="P3_6" pad="34"/>
<connect gate="G$1" pin="P3_7" pad="35"/>
<connect gate="G$1" pin="P4_0/TB0" pad="36"/>
<connect gate="G$1" pin="P4_1/TB1" pad="37"/>
<connect gate="G$1" pin="P4_2/TB2" pad="38"/>
<connect gate="G$1" pin="P4_3" pad="39"/>
<connect gate="G$1" pin="P4_4" pad="40"/>
<connect gate="G$1" pin="P4_5" pad="41"/>
<connect gate="G$1" pin="P4_6" pad="42"/>
<connect gate="G$1" pin="P4_7/TBCLK" pad="43"/>
<connect gate="G$1" pin="P5_0" pad="44"/>
<connect gate="G$1" pin="P5_1" pad="45"/>
<connect gate="G$1" pin="P5_2" pad="46"/>
<connect gate="G$1" pin="P5_3" pad="47"/>
<connect gate="G$1" pin="P5_4/MCLK" pad="48"/>
<connect gate="G$1" pin="P5_5/SMCLK" pad="49"/>
<connect gate="G$1" pin="P5_6/ACLK" pad="50"/>
<connect gate="G$1" pin="P5_7/TBOUTH/SVSOUT" pad="51"/>
<connect gate="G$1" pin="P6_0/A0" pad="59"/>
<connect gate="G$1" pin="P6_1/A1" pad="60"/>
<connect gate="G$1" pin="P6_2/A2" pad="61"/>
<connect gate="G$1" pin="P6_3/A3" pad="2"/>
<connect gate="G$1" pin="P6_4/A4" pad="3"/>
<connect gate="G$1" pin="P6_5/A5" pad="4"/>
<connect gate="G$1" pin="P6_6/A6" pad="5"/>
<connect gate="G$1" pin="P6_7/A7/SVSIN" pad="6"/>
<connect gate="G$1" pin="TCK" pad="57"/>
<connect gate="G$1" pin="TDI/TCLK" pad="55"/>
<connect gate="G$1" pin="TDO/TDI" pad="54"/>
<connect gate="G$1" pin="TMS" pad="56"/>
<connect gate="G$1" pin="VEREF+" pad="10"/>
<connect gate="G$1" pin="VREF+" pad="7"/>
<connect gate="G$1" pin="VREF--/VEREF--" pad="11"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT" pad="9"/>
<connect gate="G$1" pin="XT2IN" pad="53"/>
<connect gate="G$1" pin="XT2OUT" pad="52"/>
</connects>
<technologies>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F233TRGCT"/>
<attribute name="OC_FARNELL" value="1649429"/>
<attribute name="OC_NEWARK" value="65M1697"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F235TRGCT"/>
<attribute name="OC_FARNELL" value="1649433"/>
<attribute name="OC_NEWARK" value="65M1700"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430F24*" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;

Source: http://focus.ti.com/lit/ds/symlink/msp430f2471.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430F24X"/>
</gates>
<devices>
<device name="TRGC" package="RGC_S-PVQFV-N64">
<connects>
<connect gate="G$1" pin="!RST!/NMI" pad="58"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="AVSS" pad="62"/>
<connect gate="G$1" pin="DVCC" pad="1"/>
<connect gate="G$1" pin="DVSS" pad="63"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="P1_0/TACLK/CAOUT" pad="12"/>
<connect gate="G$1" pin="P1_1/TA0" pad="13"/>
<connect gate="G$1" pin="P1_2/TA1" pad="14"/>
<connect gate="G$1" pin="P1_3/TA2" pad="15"/>
<connect gate="G$1" pin="P1_4/SMCLK" pad="16"/>
<connect gate="G$1" pin="P1_5/TA0" pad="17"/>
<connect gate="G$1" pin="P1_6/TA1" pad="18"/>
<connect gate="G$1" pin="P1_7/TA2" pad="19"/>
<connect gate="G$1" pin="P2_0/ACLK/CA2" pad="20"/>
<connect gate="G$1" pin="P2_1/TAINCLK/CA3" pad="21"/>
<connect gate="G$1" pin="P2_2/CAOUT/TA0/CA4" pad="22"/>
<connect gate="G$1" pin="P2_3/CA0/TA1" pad="23"/>
<connect gate="G$1" pin="P2_4/CA1/TA2" pad="24"/>
<connect gate="G$1" pin="P2_5/ROSC/CA5" pad="25"/>
<connect gate="G$1" pin="P2_6/ADC12CLK/CA6" pad="26"/>
<connect gate="G$1" pin="P2_7/TA0/CA7" pad="27"/>
<connect gate="G$1" pin="P3_0/UCB0STE/UCA0CLK" pad="28"/>
<connect gate="G$1" pin="P3_1/UCB0SIMO/UCB0SDA" pad="29"/>
<connect gate="G$1" pin="P3_2/UCB0SOMI/UCB0SCL" pad="30"/>
<connect gate="G$1" pin="P3_3/UCB0CLK/UCA0STE" pad="31"/>
<connect gate="G$1" pin="P3_4/UCA0TXD/UCA0SIMO" pad="32"/>
<connect gate="G$1" pin="P3_5/UCA0RXD/UCA0SOMI" pad="33"/>
<connect gate="G$1" pin="P3_6/UCA1TXD/UCA1SIMO" pad="34"/>
<connect gate="G$1" pin="P3_7/UCA1RXD/UCA1SOMI" pad="35"/>
<connect gate="G$1" pin="P4_0/TB0" pad="36"/>
<connect gate="G$1" pin="P4_1/TB1" pad="37"/>
<connect gate="G$1" pin="P4_2/TB2" pad="38"/>
<connect gate="G$1" pin="P4_3/TB3" pad="39"/>
<connect gate="G$1" pin="P4_4/TB4" pad="40"/>
<connect gate="G$1" pin="P4_5/TB5" pad="41"/>
<connect gate="G$1" pin="P4_6/TB6" pad="42"/>
<connect gate="G$1" pin="P4_7/TBCLK" pad="43"/>
<connect gate="G$1" pin="P5_0/UCB1STE/UCA1CLK" pad="44"/>
<connect gate="G$1" pin="P5_1/UCB1SIMO/UCB1SDA" pad="45"/>
<connect gate="G$1" pin="P5_2/UCB1SOMI/UCB1SCL" pad="46"/>
<connect gate="G$1" pin="P5_3/UCB1CLK/UCA1STE" pad="47"/>
<connect gate="G$1" pin="P5_4/MCLK" pad="48"/>
<connect gate="G$1" pin="P5_5/SMCLK" pad="49"/>
<connect gate="G$1" pin="P5_6/ACLK" pad="50"/>
<connect gate="G$1" pin="P5_7/TBOUTH/SVSOUT" pad="51"/>
<connect gate="G$1" pin="P6_0/A0" pad="59"/>
<connect gate="G$1" pin="P6_1/A1" pad="60"/>
<connect gate="G$1" pin="P6_2/A2" pad="61"/>
<connect gate="G$1" pin="P6_3/A3" pad="2"/>
<connect gate="G$1" pin="P6_4/A4" pad="3"/>
<connect gate="G$1" pin="P6_5/A5" pad="4"/>
<connect gate="G$1" pin="P6_6/A6" pad="5"/>
<connect gate="G$1" pin="P6_7/A7/SVSIN" pad="6"/>
<connect gate="G$1" pin="TCK" pad="57"/>
<connect gate="G$1" pin="TDI/TCLK" pad="55"/>
<connect gate="G$1" pin="TDO/TDI" pad="54"/>
<connect gate="G$1" pin="TMS" pad="56"/>
<connect gate="G$1" pin="VEREF+" pad="10"/>
<connect gate="G$1" pin="VREF+" pad="7"/>
<connect gate="G$1" pin="VREF--/VEREF--" pad="11"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT" pad="9"/>
<connect gate="G$1" pin="XT2IN" pad="53"/>
<connect gate="G$1" pin="XT2OUT" pad="52"/>
</connects>
<technologies>
<technology name="10">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F2410TRGCT"/>
<attribute name="OC_FARNELL" value="1649436"/>
<attribute name="OC_NEWARK" value="65M1704"/>
</technology>
<technology name="47">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="49">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MSP430F24*1" prefix="IC">
<description>&lt;b&gt;MIXED SIGNAL MICROCONTROLLER&lt;/b&gt;&lt;p&gt;

Source: http://focus.ti.com/lit/ds/symlink/msp430f2471.pdf</description>
<gates>
<gate name="G$1" symbol="MSP430F24X1"/>
</gates>
<devices>
<device name="TRGC" package="RGC_S-PVQFV-N64">
<connects>
<connect gate="G$1" pin="!RST!/NMI" pad="58"/>
<connect gate="G$1" pin="AVCC" pad="64"/>
<connect gate="G$1" pin="AVSS" pad="62"/>
<connect gate="G$1" pin="DVCC" pad="1"/>
<connect gate="G$1" pin="DVSS" pad="10"/>
<connect gate="G$1" pin="DVSS@1" pad="11"/>
<connect gate="G$1" pin="DVSS@2" pad="63"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="P1_0/TACLK/CAOUT" pad="12"/>
<connect gate="G$1" pin="P1_1/TA0" pad="13"/>
<connect gate="G$1" pin="P1_2/TA1" pad="14"/>
<connect gate="G$1" pin="P1_3/TA2" pad="15"/>
<connect gate="G$1" pin="P1_4/SMCLK" pad="16"/>
<connect gate="G$1" pin="P1_5/TA0" pad="17"/>
<connect gate="G$1" pin="P1_6/TA1" pad="18"/>
<connect gate="G$1" pin="P1_7/TA2" pad="19"/>
<connect gate="G$1" pin="P2_0/ACLK/CA2" pad="20"/>
<connect gate="G$1" pin="P2_1/TAINCLK/CA3" pad="21"/>
<connect gate="G$1" pin="P2_2/CAOUT/TA0/CA4" pad="22"/>
<connect gate="G$1" pin="P2_3/CA0/TA1" pad="23"/>
<connect gate="G$1" pin="P2_4/CA1/TA2" pad="24"/>
<connect gate="G$1" pin="P2_5/ROSC/CA5" pad="25"/>
<connect gate="G$1" pin="P2_6/ADC12CLK/CA6" pad="26"/>
<connect gate="G$1" pin="P2_7/TA0/CA7" pad="27"/>
<connect gate="G$1" pin="P3_0/UCB0STE/UCA0CLK" pad="28"/>
<connect gate="G$1" pin="P3_1/UCB0SIMO/UCB0SDA" pad="29"/>
<connect gate="G$1" pin="P3_2/UCB0SOMI/UCB0SCL" pad="30"/>
<connect gate="G$1" pin="P3_3/UCB0CLK/UCA0STE" pad="31"/>
<connect gate="G$1" pin="P3_4/UCA0TXD/UCA0SIMO" pad="32"/>
<connect gate="G$1" pin="P3_5/UCA0RXD/UCA0SOMI" pad="33"/>
<connect gate="G$1" pin="P3_6/UCA1TXD/UCA1SIMO" pad="34"/>
<connect gate="G$1" pin="P3_7/UCA1RXD/UCA1SOMI" pad="35"/>
<connect gate="G$1" pin="P4_0/TB0" pad="36"/>
<connect gate="G$1" pin="P4_1/TB1" pad="37"/>
<connect gate="G$1" pin="P4_2/TB2" pad="38"/>
<connect gate="G$1" pin="P4_3/TB3" pad="39"/>
<connect gate="G$1" pin="P4_4/TB4" pad="40"/>
<connect gate="G$1" pin="P4_5/TB5" pad="41"/>
<connect gate="G$1" pin="P4_6/TB6" pad="42"/>
<connect gate="G$1" pin="P4_7/TBCLK" pad="43"/>
<connect gate="G$1" pin="P5_0/UCB1STE/UCA1CLK" pad="44"/>
<connect gate="G$1" pin="P5_1/UCB1SIMO/UCB1SDA" pad="45"/>
<connect gate="G$1" pin="P5_2/UCB1SOMI/UCB1SCL" pad="46"/>
<connect gate="G$1" pin="P5_3/UCB1CLK/UCA1STE" pad="47"/>
<connect gate="G$1" pin="P5_4/MCLK" pad="48"/>
<connect gate="G$1" pin="P5_5/SMCLK" pad="49"/>
<connect gate="G$1" pin="P5_6/ACLK" pad="50"/>
<connect gate="G$1" pin="P5_7/TBOUTH/SVSOUT" pad="51"/>
<connect gate="G$1" pin="P6_0" pad="59"/>
<connect gate="G$1" pin="P6_1" pad="60"/>
<connect gate="G$1" pin="P6_2" pad="61"/>
<connect gate="G$1" pin="P6_3" pad="2"/>
<connect gate="G$1" pin="P6_4" pad="3"/>
<connect gate="G$1" pin="P6_5" pad="4"/>
<connect gate="G$1" pin="P6_6" pad="5"/>
<connect gate="G$1" pin="P6_7/SVSIN" pad="6"/>
<connect gate="G$1" pin="RESERVED" pad="7"/>
<connect gate="G$1" pin="TCK" pad="57"/>
<connect gate="G$1" pin="TDI/TCLK" pad="55"/>
<connect gate="G$1" pin="TDO/TDI" pad="54"/>
<connect gate="G$1" pin="TMS" pad="56"/>
<connect gate="G$1" pin="XIN" pad="8"/>
<connect gate="G$1" pin="XOUT" pad="9"/>
<connect gate="G$1" pin="XT2IN" pad="53"/>
<connect gate="G$1" pin="XT2OUT" pad="52"/>
</connects>
<technologies>
<technology name="7">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1753309"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MSP430F2491TRGCT"/>
<attribute name="OC_FARNELL" value="1649447"/>
<attribute name="OC_NEWARK" value="65M1728"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CC2531" prefix="IC">
<description>&lt;b&gt;A USB Enabled System-On-Chip Solution for 2.4-GHz IEEE 802.15.4 and ZigBee&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/cc2531.pdf</description>
<gates>
<gate name="G$1" symbol="CC2531"/>
</gates>
<devices>
<device name="" package="RHA_S-PVQFN-N40">
<connects>
<connect gate="G$1" pin="AVDD@1" pad="28"/>
<connect gate="G$1" pin="AVDD@2" pad="27"/>
<connect gate="G$1" pin="AVDD@3" pad="24"/>
<connect gate="G$1" pin="AVDD@4" pad="29"/>
<connect gate="G$1" pin="AVDD@5" pad="21"/>
<connect gate="G$1" pin="AVDD@6" pad="31"/>
<connect gate="G$1" pin="DCOUPL" pad="40"/>
<connect gate="G$1" pin="DGND_USB" pad="1"/>
<connect gate="G$1" pin="DVDD@1" pad="39"/>
<connect gate="G$1" pin="DVDD@2" pad="10"/>
<connect gate="G$1" pin="DVDD_USB" pad="4"/>
<connect gate="G$1" pin="GND" pad="EXP"/>
<connect gate="G$1" pin="P0_0" pad="19"/>
<connect gate="G$1" pin="P0_1" pad="18"/>
<connect gate="G$1" pin="P0_2" pad="17"/>
<connect gate="G$1" pin="P0_3" pad="16"/>
<connect gate="G$1" pin="P0_4" pad="15"/>
<connect gate="G$1" pin="P0_5" pad="14"/>
<connect gate="G$1" pin="P0_6" pad="13"/>
<connect gate="G$1" pin="P0_7" pad="12"/>
<connect gate="G$1" pin="P1_0" pad="11"/>
<connect gate="G$1" pin="P1_1" pad="9"/>
<connect gate="G$1" pin="P1_2" pad="8"/>
<connect gate="G$1" pin="P1_3" pad="7"/>
<connect gate="G$1" pin="P1_4" pad="6"/>
<connect gate="G$1" pin="P1_5" pad="5"/>
<connect gate="G$1" pin="P1_6" pad="38"/>
<connect gate="G$1" pin="P1_7" pad="37"/>
<connect gate="G$1" pin="P2_0" pad="36"/>
<connect gate="G$1" pin="P2_1" pad="35"/>
<connect gate="G$1" pin="P2_2" pad="34"/>
<connect gate="G$1" pin="P2_3/XOSC32K_Q2" pad="33"/>
<connect gate="G$1" pin="P2_4/XOSC32K_Q1" pad="32"/>
<connect gate="G$1" pin="RBIAS" pad="30"/>
<connect gate="G$1" pin="RESET_N" pad="20"/>
<connect gate="G$1" pin="RF_N" pad="26"/>
<connect gate="G$1" pin="RF_P" pad="25"/>
<connect gate="G$1" pin="USB_N" pad="3"/>
<connect gate="G$1" pin="USB_P" pad="2"/>
<connect gate="G$1" pin="XOSC_Q1" pad="22"/>
<connect gate="G$1" pin="XOSC_Q2" pad="23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CC2531F256RHAT"/>
<attribute name="OC_FARNELL" value="1776351"/>
<attribute name="OC_NEWARK" value="34R2713"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISO1176" prefix="IC">
<description>&lt;b&gt;ISOLATED RS-485 PROFIBUS TRANSCEIVER&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://focus.ti.com/docs/prod/folders/print/iso1176.html"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ISO1176"/>
</gates>
<devices>
<device name="" package="SO-16DW">
<connects>
<connect gate="G$1" pin="!RE" pad="4"/>
<connect gate="G$1" pin="A" pad="12"/>
<connect gate="G$1" pin="B" pad="13"/>
<connect gate="G$1" pin="D" pad="6"/>
<connect gate="G$1" pin="DE" pad="5"/>
<connect gate="G$1" pin="GND1@1" pad="2"/>
<connect gate="G$1" pin="GND1@2" pad="8"/>
<connect gate="G$1" pin="GND2@1" pad="15"/>
<connect gate="G$1" pin="GND2@2" pad="9"/>
<connect gate="G$1" pin="ISODE" pad="10"/>
<connect gate="G$1" pin="NC@1" pad="14"/>
<connect gate="G$1" pin="NC@2" pad="11"/>
<connect gate="G$1" pin="PV" pad="7"/>
<connect gate="G$1" pin="R" pad="3"/>
<connect gate="G$1" pin="VCC1" pad="1"/>
<connect gate="G$1" pin="VCC2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ISO1176DW"/>
<attribute name="OC_FARNELL" value="1755037"/>
<attribute name="OC_NEWARK" value="13N4111"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1232LP" prefix="IC">
<description>&lt;b&gt;Low Power MicroMonitor Chip&lt;/b&gt;&lt;p&gt;
Source: DALLAS SEMICONDUCTOR .. 1232lp.pdf</description>
<gates>
<gate name="G$1" symbol="DS1232LP"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="!PBRST" pad="1"/>
<connect gate="G$1" pin="!RST" pad="6"/>
<connect gate="G$1" pin="!ST" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="TD" pad="2"/>
<connect gate="G$1" pin="TOL" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS1232LP+"/>
<attribute name="OC_FARNELL" value="1187997"/>
<attribute name="OC_NEWARK" value="68K3327"/>
</technology>
</technologies>
</device>
<device name="S-2" package="SO-08">
<connects>
<connect gate="G$1" pin="!PBRST" pad="1"/>
<connect gate="G$1" pin="!RST" pad="6"/>
<connect gate="G$1" pin="!ST" pad="7"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="RST" pad="5"/>
<connect gate="G$1" pin="TD" pad="2"/>
<connect gate="G$1" pin="TOL" pad="3"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="DALLAS SEMICONDUCTOR"/>
<attribute name="MPN" value="DS1232LPS-2"/>
<attribute name="OC_FARNELL" value="9724877"/>
<attribute name="OC_NEWARK" value="06F4304"/>
</technology>
</technologies>
</device>
<device name="S" package="SO-16DW">
<connects>
<connect gate="G$1" pin="!PBRST" pad="2"/>
<connect gate="G$1" pin="!RST" pad="11"/>
<connect gate="G$1" pin="!ST" pad="13"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="RST" pad="9"/>
<connect gate="G$1" pin="TD" pad="4"/>
<connect gate="G$1" pin="TOL" pad="6"/>
<connect gate="G$1" pin="VCC" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS1232LPS+"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="99K1954"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS5410" prefix="IC">
<description>&lt;b&gt;1-A, WIDE INPUT RANGE, STEP-DOWN SWIFT? CONVERTER&lt;/b&gt;&lt;p&gt;
Source: U7 Texas TPS5410 Step Down Converter.pdf</description>
<gates>
<gate name="P" symbol="TPS5410"/>
</gates>
<devices>
<device name="" package="D_R-PDSO-G08">
<connects>
<connect gate="P" pin="BOOT" pad="1"/>
<connect gate="P" pin="ENA" pad="5"/>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="PH" pad="8"/>
<connect gate="P" pin="VIN" pad="7"/>
<connect gate="P" pin="VSENSE" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TPS5410DR"/>
<attribute name="OC_FARNELL" value="1329596"/>
<attribute name="OC_NEWARK" value="18M3223"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ78PL114" prefix="IC">
<description>&lt;b&gt;PowerLAN (TM) Master Gateway Battery Management Controller With PowerPump(TM) Cell Balancing Technology&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://focus.ti.com/lit/ds/symlink/bq78pl114.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="BQ78PL114"/>
</gates>
<devices>
<device name="" package="P-QFP48-7X7MM">
<connects>
<connect gate="G$1" pin="CCBAT" pad="6"/>
<connect gate="G$1" pin="CCPACK" pad="7"/>
<connect gate="G$1" pin="CHG" pad="1"/>
<connect gate="G$1" pin="CSBAT" pad="9"/>
<connect gate="G$1" pin="CSPACK" pad="10"/>
<connect gate="G$1" pin="DSG" pad="2"/>
<connect gate="G$1" pin="EFCIC" pad="4"/>
<connect gate="G$1" pin="EFCID" pad="5"/>
<connect gate="G$1" pin="EXP" pad="EXP"/>
<connect gate="G$1" pin="LED1" pad="32"/>
<connect gate="G$1" pin="LED2" pad="33"/>
<connect gate="G$1" pin="LED3" pad="34"/>
<connect gate="G$1" pin="LED4" pad="35"/>
<connect gate="G$1" pin="LED5" pad="36"/>
<connect gate="G$1" pin="LEDEN" pad="31"/>
<connect gate="G$1" pin="NC" pad="28"/>
<connect gate="G$1" pin="NC-I" pad="27"/>
<connect gate="G$1" pin="NC-IO" pad="26"/>
<connect gate="G$1" pin="NC@1" pad="29"/>
<connect gate="G$1" pin="OSCI" pad="11"/>
<connect gate="G$1" pin="OSCO" pad="12"/>
<connect gate="G$1" pin="P-LAN" pad="24"/>
<connect gate="G$1" pin="P1N" pad="15"/>
<connect gate="G$1" pin="P2N" pad="17"/>
<connect gate="G$1" pin="P2S" pad="16"/>
<connect gate="G$1" pin="P3N" pad="21"/>
<connect gate="G$1" pin="P3S" pad="20"/>
<connect gate="G$1" pin="P4N" pad="23"/>
<connect gate="G$1" pin="P4S" pad="22"/>
<connect gate="G$1" pin="PRE" pad="3"/>
<connect gate="G$1" pin="RSTN" pad="25"/>
<connect gate="G$1" pin="SDI1" pad="14"/>
<connect gate="G$1" pin="SDI3" pad="19"/>
<connect gate="G$1" pin="SDO0" pad="13"/>
<connect gate="G$1" pin="SDO2" pad="18"/>
<connect gate="G$1" pin="SMBCLK" pad="37"/>
<connect gate="G$1" pin="SMBDAT" pad="38"/>
<connect gate="G$1" pin="SPROT" pad="30"/>
<connect gate="G$1" pin="V1" pad="47"/>
<connect gate="G$1" pin="V2" pad="44"/>
<connect gate="G$1" pin="V3" pad="42"/>
<connect gate="G$1" pin="V4" pad="39"/>
<connect gate="G$1" pin="VLDO1" pad="8"/>
<connect gate="G$1" pin="VLDO2" pad="43"/>
<connect gate="G$1" pin="VSS" pad="48"/>
<connect gate="G$1" pin="XT1" pad="46"/>
<connect gate="G$1" pin="XT2" pad="45"/>
<connect gate="G$1" pin="XT3" pad="41"/>
<connect gate="G$1" pin="XT4" pad="40"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="BQ78PL114RGZR"/>
<attribute name="OC_FARNELL" value="1684746"/>
<attribute name="OC_NEWARK" value="12P8640"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TMS320C5515" prefix="IC">
<description>&lt;b&gt;TMS320C5515&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 36&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://focus.ti.com/lit/ds/symlink/tms320c5515.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TMS320C5515"/>
</gates>
<devices>
<device name="" package="ZCH(S-PBGA-N196)">
<connects>
<connect gate="G$1" pin="ANA_LDOO" pad="A12"/>
<connect gate="G$1" pin="BG_CAP" pad="B13"/>
<connect gate="G$1" pin="CLKIN" pad="A8"/>
<connect gate="G$1" pin="CLKOUT" pad="A7"/>
<connect gate="G$1" pin="CLK_SEL" pad="C7"/>
<connect gate="G$1" pin="CVDD" pad="L5"/>
<connect gate="G$1" pin="CVDD@1" pad="J5"/>
<connect gate="G$1" pin="CVDD@2" pad="K9"/>
<connect gate="G$1" pin="CVDD@3" pad="L14"/>
<connect gate="G$1" pin="CVDD@4" pad="M10"/>
<connect gate="G$1" pin="CVDDRTC" pad="C8"/>
<connect gate="G$1" pin="DSP_LDOO" pad="E10"/>
<connect gate="G$1" pin="DSP_LDO_EN" pad="D12"/>
<connect gate="G$1" pin="DVDDEMIF" pad="P2"/>
<connect gate="G$1" pin="DVDDEMIF@1" pad="A5"/>
<connect gate="G$1" pin="DVDDEMIF@2" pad="E9"/>
<connect gate="G$1" pin="DVDDEMIF@3" pad="F9"/>
<connect gate="G$1" pin="DVDDEMIF@4" pad="G12"/>
<connect gate="G$1" pin="DVDDEMIF@5" pad="J2"/>
<connect gate="G$1" pin="DVDDEMIF@6" pad="J4"/>
<connect gate="G$1" pin="DVDDEMIF@7" pad="K8"/>
<connect gate="G$1" pin="DVDDIO" pad="P8"/>
<connect gate="G$1" pin="DVDDIO@1" pad="L11"/>
<connect gate="G$1" pin="DVDDIO@2" pad="M2"/>
<connect gate="G$1" pin="DVDDRTC" pad="F8"/>
<connect gate="G$1" pin="EMU0" pad="L6"/>
<connect gate="G$1" pin="EM_A[0]" pad="B2"/>
<connect gate="G$1" pin="EM_A[10]" pad="L2"/>
<connect gate="G$1" pin="EM_A[11]/_ALE_" pad="K2"/>
<connect gate="G$1" pin="EM_A[13]" pad="L1"/>
<connect gate="G$1" pin="EM_A[16]/GP[22]" pad="E2"/>
<connect gate="G$1" pin="EM_A[16]/GP[22]@1" pad="E5"/>
<connect gate="G$1" pin="EM_A[17]/GP[23]@1" pad="F6"/>
<connect gate="G$1" pin="EM_A[18]/GP[24]@1" pad="G8"/>
<connect gate="G$1" pin="EM_A[19]/GP[25]@1" pad="G11"/>
<connect gate="G$1" pin="EM_A[1]" pad="C2"/>
<connect gate="G$1" pin="EM_A[20]/GP[26]@1" pad="K6"/>
<connect gate="G$1" pin="EM_A[2]" pad="E1"/>
<connect gate="G$1" pin="EM_A[3]" pad="D2"/>
<connect gate="G$1" pin="EM_A[4]" pad="C1"/>
<connect gate="G$1" pin="EM_A[5]" pad="D1"/>
<connect gate="G$1" pin="EM_A[8]" pad="J1"/>
<connect gate="G$1" pin="EM_BA[0]" pad="A1"/>
<connect gate="G$1" pin="EM_BA[1]" pad="B1"/>
<connect gate="G$1" pin="EM_CS0" pad="B3"/>
<connect gate="G$1" pin="EM_CS1" pad="A4"/>
<connect gate="G$1" pin="EM_CS2" pad="C5"/>
<connect gate="G$1" pin="EM_CS3" pad="M4"/>
<connect gate="G$1" pin="EM_CS4" pad="C3"/>
<connect gate="G$1" pin="EM_CS5" pad="A3"/>
<connect gate="G$1" pin="EM_DQM0" pad="B5"/>
<connect gate="G$1" pin="EM_DQM1" pad="P1"/>
<connect gate="G$1" pin="EM_D[0]" pad="G3"/>
<connect gate="G$1" pin="EM_D[10]" pad="D3"/>
<connect gate="G$1" pin="EM_D[11]" pad="C4"/>
<connect gate="G$1" pin="EM_D[13]" pad="K4"/>
<connect gate="G$1" pin="EM_D[14]" pad="K3"/>
<connect gate="G$1" pin="EM_D[3]" pad="D4"/>
<connect gate="G$1" pin="EM_D[4]" pad="L4"/>
<connect gate="G$1" pin="EM_D[6]" pad="K5"/>
<connect gate="G$1" pin="EM_D[7]" pad="H3"/>
<connect gate="G$1" pin="EM_D[8]" pad="E3"/>
<connect gate="G$1" pin="EM_D[9]" pad="F4"/>
<connect gate="G$1" pin="EM_OE" pad="E4"/>
<connect gate="G$1" pin="EM_R/W" pad="B6"/>
<connect gate="G$1" pin="EM_SDCAS" pad="B4"/>
<connect gate="G$1" pin="EM_SDRAS" pad="A6"/>
<connect gate="G$1" pin="EM_WAIT2" pad="D5"/>
<connect gate="G$1" pin="EM_WAIT4" pad="G1"/>
<connect gate="G$1" pin="EM_WAIT5" pad="H4"/>
<connect gate="G$1" pin="EM_WE" pad="H1"/>
<connect gate="G$1" pin="GPAIN0" pad="D10"/>
<connect gate="G$1" pin="GPAIN1" pad="A11"/>
<connect gate="G$1" pin="GPAIN2" pad="B11"/>
<connect gate="G$1" pin="INT0" pad="C6"/>
<connect gate="G$1" pin="INT1" pad="E7"/>
<connect gate="G$1" pin="LCD_CS0_E0/" pad="P4"/>
<connect gate="G$1" pin="LCD_D8]/I2S2_CLK/GP[18]/SPI_CLK" pad="N10"/>
<connect gate="G$1" pin="LCD_D[0]/SPI_RX" pad="P6"/>
<connect gate="G$1" pin="LCD_D[12]/UART_RTS/GP[28]/I2S3_CLK" pad="N12"/>
<connect gate="G$1" pin="LCD_D[15]/UART_TXD/GP[31]/I2S3_DX" pad="P14"/>
<connect gate="G$1" pin="LCD_D[1]/SPI_TX" pad="N6"/>
<connect gate="G$1" pin="LCD_D[2]/GP[12]" pad="P7"/>
<connect gate="G$1" pin="LCD_D[4]/GP[14]" pad="N8"/>
<connect gate="G$1" pin="LCD_D[7]/GP[17]" pad="P10"/>
<connect gate="G$1" pin="LCD_D[9]/I2S2_FS/GP[19]/SPI_CS0" pad="P11"/>
<connect gate="G$1" pin="LCD_EN_RDB/" pad="N3"/>
<connect gate="G$1" pin="LCD_RW_WRB/" pad="P5"/>
<connect gate="G$1" pin="LDOI" pad="B12"/>
<connect gate="G$1" pin="LDOI@1" pad="G4"/>
<connect gate="G$1" pin="LDOI@2" pad="G5"/>
<connect gate="G$1" pin="MMC0_CLK/I2S0_CLK/GP[0]" pad="L10"/>
<connect gate="G$1" pin="MMC0_CLK/I2S0_CLK/GP[0]@1" pad="N4"/>
<connect gate="G$1" pin="MMC0_CLK/I2S0_CLK/GP[0]@2" pad="N5"/>
<connect gate="G$1" pin="MMC0_CMD/I2S0_FS/GP[1]" pad="M11"/>
<connect gate="G$1" pin="MMC0_D0/I2S0_DX/GP[2]" pad="L9"/>
<connect gate="G$1" pin="MMC0_D0/I2S0_DX/GP[2]@1" pad="N1"/>
<connect gate="G$1" pin="MMC0_D0/I2S0_DX/GP[2]@2" pad="N2"/>
<connect gate="G$1" pin="MMC0_D1/I2S0_RX/GP[3]@1" pad="P12"/>
<connect gate="G$1" pin="MMC0_D1/I2S0_RX/GP[3]@2" pad="P13"/>
<connect gate="G$1" pin="MMC0_D2/GP[4]@1" pad="N9"/>
<connect gate="G$1" pin="MMC0_D3/GP[5]@1" pad="N7"/>
<connect gate="G$1" pin="MMC1_CLK/I2S1_CLK/GP[6]" pad="M13"/>
<connect gate="G$1" pin="MMC1_CMD/I2S1_FS/GP[7]@1" pad="N13"/>
<connect gate="G$1" pin="MMC1_CMD/I2S1_FS/GP[7]@2" pad="N14"/>
<connect gate="G$1" pin="MMC1_D0/2S1_DX/GP[8]" pad="M14"/>
<connect gate="G$1" pin="MMC1_D1/I2S1_RX/GP[9]" pad="M12"/>
<connect gate="G$1" pin="MMC1_D2/GP[10]" pad="K14"/>
<connect gate="G$1" pin="MMC1_D2/GP[10]@1" pad="M5"/>
<connect gate="G$1" pin="MMC1_D3/GP[11]@1" pad="N11"/>
<connect gate="G$1" pin="RESET" pad="D6"/>
<connect gate="G$1" pin="RSV0" pad="C12"/>
<connect gate="G$1" pin="RSV1" pad="J10"/>
<connect gate="G$1" pin="RSV3" pad="D14"/>
<connect gate="G$1" pin="RSV4" pad="C14"/>
<connect gate="G$1" pin="RSV5" pad="C13"/>
<connect gate="G$1" pin="RTC_XI" pad="B9"/>
<connect gate="G$1" pin="RTC_XO" pad="A9"/>
<connect gate="G$1" pin="SCL" pad="B7"/>
<connect gate="G$1" pin="SDA" pad="B8"/>
<connect gate="G$1" pin="TCK" pad="M6"/>
<connect gate="G$1" pin="TDI" pad="L7"/>
<connect gate="G$1" pin="TDO" pad="M7"/>
<connect gate="G$1" pin="TMS" pad="L8"/>
<connect gate="G$1" pin="TRST" pad="M9"/>
<connect gate="G$1" pin="USB_DM" pad="J14"/>
<connect gate="G$1" pin="USB_DP" pad="H14"/>
<connect gate="G$1" pin="USB_LDOO" pad="F12"/>
<connect gate="G$1" pin="USB_R1" pad="G9"/>
<connect gate="G$1" pin="USB_VBUS" pad="J12"/>
<connect gate="G$1" pin="USB_VDD1P3@1" pad="L3"/>
<connect gate="G$1" pin="USB_VDDA1P3" pad="H10"/>
<connect gate="G$1" pin="USB_VDDA1P3@1" pad="J9"/>
<connect gate="G$1" pin="USB_VDDA3P3" pad="H12"/>
<connect gate="G$1" pin="USB_VDDA3P3@1" pad="J13"/>
<connect gate="G$1" pin="USB_VDDOSC@1" pad="H9"/>
<connect gate="G$1" pin="USB_VDDPLL@1" pad="H2"/>
<connect gate="G$1" pin="USB_VSS1P3" pad="H13"/>
<connect gate="G$1" pin="USB_VSS1P3@1" pad="K1"/>
<connect gate="G$1" pin="USB_VSSA1P3@1" pad="J7"/>
<connect gate="G$1" pin="USB_VSSA3P3" pad="H11"/>
<connect gate="G$1" pin="USB_VSSA3P3@1" pad="J11"/>
<connect gate="G$1" pin="USB_VSSOSC" pad="F11"/>
<connect gate="G$1" pin="USB_VSSOSC@1" pad="G2"/>
<connect gate="G$1" pin="USB_VSSPLL@1" pad="H7"/>
<connect gate="G$1" pin="USB_VSSREF" pad="G10"/>
<connect gate="G$1" pin="USB_VSSREF@1" pad="H5"/>
<connect gate="G$1" pin="VDDA_ANA" pad="A10"/>
<connect gate="G$1" pin="VDDA_PLL" pad="C10"/>
<connect gate="G$1" pin="VDDA_PLL@1" pad="C11"/>
<connect gate="G$1" pin="VSS" pad="K13"/>
<connect gate="G$1" pin="VSS@1" pad="A14"/>
<connect gate="G$1" pin="VSS@10" pad="F14"/>
<connect gate="G$1" pin="VSS@11" pad="G13"/>
<connect gate="G$1" pin="VSS@12" pad="G14"/>
<connect gate="G$1" pin="VSS@13" pad="J3"/>
<connect gate="G$1" pin="VSS@14" pad="K10"/>
<connect gate="G$1" pin="VSS@15" pad="K11"/>
<connect gate="G$1" pin="VSS@16" pad="K12"/>
<connect gate="G$1" pin="VSS@17" pad="L12"/>
<connect gate="G$1" pin="VSS@18" pad="L13"/>
<connect gate="G$1" pin="VSS@19" pad="M1"/>
<connect gate="G$1" pin="VSS@2" pad="D8"/>
<connect gate="G$1" pin="VSS@20" pad="M3"/>
<connect gate="G$1" pin="VSS@3" pad="D13"/>
<connect gate="G$1" pin="VSS@4" pad="E12"/>
<connect gate="G$1" pin="VSS@5" pad="E14"/>
<connect gate="G$1" pin="VSS@6" pad="F1"/>
<connect gate="G$1" pin="VSS@7" pad="F2"/>
<connect gate="G$1" pin="VSS@8" pad="F3"/>
<connect gate="G$1" pin="VSS@9" pad="F13"/>
<connect gate="G$1" pin="VSSA_ANA" pad="B10"/>
<connect gate="G$1" pin="VSSA_ANA@1" pad="B14"/>
<connect gate="G$1" pin="VSSA_PLL" pad="D9"/>
<connect gate="G$1" pin="VSSA_PLL@1" pad="D11"/>
<connect gate="G$1" pin="VSSRTC" pad="C9"/>
<connect gate="G$1" pin="WAKEUP" pad="E8"/>
<connect gate="G$1" pin="XF" pad="M8"/>
<connect gate="G$1" pin="XF@1" pad="P9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC*84" prefix="IC">
<description>&lt;b&gt;CURRENT-MODE PWM CONTROLLER&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://focus.ti.com/lit/ds/symlink/uc2843.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="UC384D"/>
</gates>
<devices>
<device name="2D" package="D_R-PDSO-G14">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="ISENSE" pad="5"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="REF" pad="14"/>
<connect gate="G$1" pin="RT/CT" pad="7"/>
<connect gate="G$1" pin="VC" pad="11"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VFB" pad="3"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC2842D8TR"/>
<attribute name="OC_FARNELL" value="1413230"/>
</technology>
<technology name="3">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC3842D"/>
<attribute name="OC_FARNELL" value="1652427"/>
</technology>
</technologies>
</device>
<device name="3D" package="D_R-PDSO-G14">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="ISENSE" pad="5"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="REF" pad="14"/>
<connect gate="G$1" pin="RT/CT" pad="7"/>
<connect gate="G$1" pin="VC" pad="11"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VFB" pad="3"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC2843D"/>
<attribute name="OC_FARNELL" value="1388056"/>
</technology>
<technology name="3">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC3843DG4"/>
<attribute name="OC_FARNELL" value="1234952"/>
</technology>
</technologies>
</device>
<device name="4D" package="D_R-PDSO-G14">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="ISENSE" pad="5"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="REF" pad="14"/>
<connect gate="G$1" pin="RT/CT" pad="7"/>
<connect gate="G$1" pin="VC" pad="11"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VFB" pad="3"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="UC3844BDG"/>
<attribute name="OC_FARNELL" value="1228725"/>
</technology>
</technologies>
</device>
<device name="5D" package="D_R-PDSO-G14">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="9"/>
<connect gate="G$1" pin="ISENSE" pad="5"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="PGND" pad="8"/>
<connect gate="G$1" pin="REF" pad="14"/>
<connect gate="G$1" pin="RT/CT" pad="7"/>
<connect gate="G$1" pin="VC" pad="11"/>
<connect gate="G$1" pin="VCC" pad="12"/>
<connect gate="G$1" pin="VFB" pad="3"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC2845DG4"/>
<attribute name="OC_FARNELL" value="1234881"/>
</technology>
<technology name="3">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC3845DG4"/>
<attribute name="OC_FARNELL" value="1234967"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="UC*84?" prefix="IC">
<description>&lt;b&gt;CURRENT-MODE PWM CONTROLLER&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://focus.ti.com/lit/ds/symlink/uc2843.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="UC384P"/>
</gates>
<devices>
<device name="2P" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value="NTE ELECTRONICS"/>
<attribute name="MPN" value="NTE7096"/>
<attribute name="OC_FARNELL" value="4531085"/>
</technology>
</technologies>
</device>
<device name="3P" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
</technologies>
</device>
<device name="4P" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5P" package="DIL08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
</technologies>
</device>
<device name="2D" package="D_R-PDSO-G08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC2842D8TR"/>
<attribute name="OC_FARNELL" value="1413230"/>
</technology>
<technology name="3">
<attribute name="MF" value="UNITRODE"/>
<attribute name="MPN" value="UC3842AD8"/>
<attribute name="OC_FARNELL" value="1101423"/>
</technology>
</technologies>
</device>
<device name="3D" package="D_R-PDSO-G08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC2843D8G4"/>
<attribute name="OC_FARNELL" value="1207369"/>
</technology>
<technology name="3">
<attribute name="MF" value="UNITRODE"/>
<attribute name="MPN" value="UC3843D8"/>
<attribute name="OC_FARNELL" value="1101424"/>
</technology>
</technologies>
</device>
<device name="4D" package="D_R-PDSO-G08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value="ON SEMICONDUCTOR"/>
<attribute name="MPN" value="UC3844BD1G"/>
<attribute name="OC_FARNELL" value="1211129"/>
</technology>
</technologies>
</device>
<device name="5D" package="D_R-PDSO-G08">
<connects>
<connect gate="G$1" pin="COMP" pad="1"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ISENSE" pad="3"/>
<connect gate="G$1" pin="OUT" pad="6"/>
<connect gate="G$1" pin="REF" pad="8"/>
<connect gate="G$1" pin="RT/CT" pad="4"/>
<connect gate="G$1" pin="VCC" pad="7"/>
<connect gate="G$1" pin="VFB" pad="2"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
<technology name="3">
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="MPN" value="UC3845D8G4"/>
<attribute name="OC_FARNELL" value="1219426"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CC2540" prefix="IC">
<description>&lt;b&gt;2.4-GHz Bluetooth® low energy System-on-Chip&lt;/b&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 39&lt;/i&gt;&lt;br&gt;
Source: cc2540.txt</description>
<gates>
<gate name="G$1" symbol="CC2540"/>
<gate name="EXP" symbol="EXP-16"/>
</gates>
<devices>
<device name="" package="QFN40-6X6">
<connects>
<connect gate="EXP" pin="EXP16@1" pad="EXP@1"/>
<connect gate="EXP" pin="EXP16@10" pad="EXP@10"/>
<connect gate="EXP" pin="EXP16@11" pad="EXP@11"/>
<connect gate="EXP" pin="EXP16@12" pad="EXP@12"/>
<connect gate="EXP" pin="EXP16@13" pad="EXP@13"/>
<connect gate="EXP" pin="EXP16@14" pad="EXP@14"/>
<connect gate="EXP" pin="EXP16@15" pad="EXP@15"/>
<connect gate="EXP" pin="EXP16@16" pad="EXP@16"/>
<connect gate="EXP" pin="EXP16@2" pad="EXP@2"/>
<connect gate="EXP" pin="EXP16@3" pad="EXP@3"/>
<connect gate="EXP" pin="EXP16@4" pad="EXP@4"/>
<connect gate="EXP" pin="EXP16@5" pad="EXP@5"/>
<connect gate="EXP" pin="EXP16@6" pad="EXP@6"/>
<connect gate="EXP" pin="EXP16@7" pad="EXP@7"/>
<connect gate="EXP" pin="EXP16@8" pad="EXP@8"/>
<connect gate="EXP" pin="EXP16@9" pad="EXP@9"/>
<connect gate="G$1" pin="AVDD1" pad="28"/>
<connect gate="G$1" pin="AVDD2" pad="27"/>
<connect gate="G$1" pin="AVDD3" pad="24"/>
<connect gate="G$1" pin="AVDD4" pad="29"/>
<connect gate="G$1" pin="AVDD5" pad="21"/>
<connect gate="G$1" pin="AVDD6" pad="31"/>
<connect gate="G$1" pin="DCOUPL" pad="40"/>
<connect gate="G$1" pin="DGND_USB" pad="1"/>
<connect gate="G$1" pin="DVDD1" pad="39"/>
<connect gate="G$1" pin="DVDD2" pad="10"/>
<connect gate="G$1" pin="DVDD_USB" pad="4"/>
<connect gate="G$1" pin="P0_0" pad="19"/>
<connect gate="G$1" pin="P0_1" pad="18"/>
<connect gate="G$1" pin="P0_2" pad="17"/>
<connect gate="G$1" pin="P0_3" pad="16"/>
<connect gate="G$1" pin="P0_4" pad="15"/>
<connect gate="G$1" pin="P0_5" pad="14"/>
<connect gate="G$1" pin="P0_6" pad="13"/>
<connect gate="G$1" pin="P0_7" pad="12"/>
<connect gate="G$1" pin="P1_0" pad="11"/>
<connect gate="G$1" pin="P1_1" pad="9"/>
<connect gate="G$1" pin="P1_2" pad="8"/>
<connect gate="G$1" pin="P1_3" pad="7"/>
<connect gate="G$1" pin="P1_4" pad="6"/>
<connect gate="G$1" pin="P1_5" pad="5"/>
<connect gate="G$1" pin="P1_6" pad="38"/>
<connect gate="G$1" pin="P1_7" pad="37"/>
<connect gate="G$1" pin="P2_0" pad="36"/>
<connect gate="G$1" pin="P2_1" pad="35"/>
<connect gate="G$1" pin="P2_2" pad="34"/>
<connect gate="G$1" pin="P2_3/XOSC32K_Q2" pad="33"/>
<connect gate="G$1" pin="P2_4/XOSC32K_Q1" pad="32"/>
<connect gate="G$1" pin="RBIAS" pad="30"/>
<connect gate="G$1" pin="RESET_N" pad="20"/>
<connect gate="G$1" pin="RF_N" pad="26"/>
<connect gate="G$1" pin="RF_P" pad="25"/>
<connect gate="G$1" pin="USB_N" pad="3"/>
<connect gate="G$1" pin="USB_P" pad="2"/>
<connect gate="G$1" pin="XOSC_Q1" pad="22"/>
<connect gate="G$1" pin="XOSC_Q2" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SWRA092B" prefix="ANT">
<description>&lt;b&gt;Compact Reach XtendTM Bluetooth®, 802.11b/g WLAN Chip Antenna&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/an/swra092b/swra092b.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ANTENNA"/>
</gates>
<devices>
<device name="" package="SWRA092B">
<connects>
<connect gate="G$1" pin="ANTENNA" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS62120" prefix="IC">
<description>&lt;b&gt;15V, 75mA High Efficient Buck Converter&lt;/b&gt;&lt;p&gt;
Source: tps62120.pdf (www.ti.com)</description>
<gates>
<gate name="G$1" symbol="TPS62120"/>
</gates>
<devices>
<device name="" package="DCN-R-PDSO-G8">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="5"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="PG" pad="6"/>
<connect gate="G$1" pin="SGND" pad="4"/>
<connect gate="G$1" pin="SW" pad="7"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BQ24022" prefix="IC">
<description>&lt;b&gt;SINGLE-CHIP, LI-ION AND LI-POL CHARGER IC&lt;/b&gt; WITH AUTONOMOUS USB-PORT AND AC-ADAPTER SUPPLY MANAGEMENT (bqTINY™-II)&lt;p&gt;
Source: bq24022.pdf (www.ti.com)</description>
<gates>
<gate name="G$1" symbol="BQ24022"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="DRC-S-PVSON-N10">
<connects>
<connect gate="G$1" pin="1CE" pad="8"/>
<connect gate="G$1" pin="AC" pad="1"/>
<connect gate="G$1" pin="ISET1" pad="6"/>
<connect gate="G$1" pin="ISET2" pad="7"/>
<connect gate="G$1" pin="OUT" pad="10"/>
<connect gate="G$1" pin="STAT1" pad="3"/>
<connect gate="G$1" pin="STAT2" pad="4"/>
<connect gate="G$1" pin="TS" pad="9"/>
<connect gate="G$1" pin="USB" pad="2"/>
<connect gate="G$1" pin="VSS" pad="5"/>
<connect gate="TH" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC4502" prefix="IC">
<description>&lt;b&gt;FAMILY OF SELF-CALIBRATING (Self-Cal TM) PRECISION CMOS RAIL-TO-RAIL OUTPUT OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/tlc4502.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="A" symbol="TLC450X"/>
<gate name="B" symbol="TLC450X"/>
<gate name="P" symbol="TLC450P"/>
</gates>
<devices>
<device name="JG" package="DIL08">
<connects>
<connect gate="A" pin="+" pad="3"/>
<connect gate="A" pin="-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+" pad="5"/>
<connect gate="B" pin="-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="D_R-PDSO-G08">
<connects>
<connect gate="A" pin="+" pad="3"/>
<connect gate="A" pin="-" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+" pad="5"/>
<connect gate="B" pin="-" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLC4501" prefix="IC">
<description>&lt;b&gt;FAMILY OF SELF-CALIBRATING (Self-Cal TM) PRECISION CMOS RAIL-TO-RAIL OUTPUT OPERATIONAL AMPLIFIERS&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/tlc4502.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="A" symbol="TLC450X"/>
<gate name="P" symbol="TLC450P"/>
</gates>
<devices>
<device name="D" package="D_R-PDSO-G08">
<connects>
<connect gate="A" pin="+" pad="7"/>
<connect gate="A" pin="-" pad="4"/>
<connect gate="A" pin="OUT" pad="6"/>
<connect gate="P" pin="V+" pad="3"/>
<connect gate="P" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TPS6306*" prefix="IC">
<description>&lt;b&gt;HIGH INPUT VOLTAGE BUCK-BOOST CONVERTER WITH 2A SWITCH CURRENT&lt;/b&gt;&lt;p&gt;
Source: http://www.ti.com/lit/ds/symlink/tps63060.pdf</description>
<gates>
<gate name="G$1" symbol="TPS63060"/>
</gates>
<devices>
<device name="" package="DSC-S-PWSON-N10">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="FB" pad="8"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="L1" pad="1"/>
<connect gate="G$1" pin="L2" pad="10"/>
<connect gate="G$1" pin="PG" pad="5"/>
<connect gate="G$1" pin="PGND" pad="PP PP@1 PP@2 PP@3 PP@4 PP@5 PP@7 PP@8 PP@9 PP@10" route="any"/>
<connect gate="G$1" pin="PS/SYNC" pad="4"/>
<connect gate="G$1" pin="VAUX" pad="6"/>
<connect gate="G$1" pin="VIN" pad="2"/>
<connect gate="G$1" pin="VOUT" pad="9"/>
</connects>
<technologies>
<technology name="0"/>
<technology name="1"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM3401" prefix="IC">
<description>&lt;b&gt;Hysteretic PFET Controller for High Power LED Drive&lt;/b&gt;&lt;p&gt;
APPLICATIONS:&lt;br&gt;
LED Driver&lt;br&gt;
Battery Charger&lt;p&gt;
Source: http://www.ti.com/lit/ds/symlink/lm3401.pdf</description>
<gates>
<gate name="G$1" symbol="LM3401"/>
</gates>
<devices>
<device name="" package="S-PDSO-G08">
<connects>
<connect gate="G$1" pin="CS" pad="1"/>
<connect gate="G$1" pin="DIM" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="HG" pad="6"/>
<connect gate="G$1" pin="HYS" pad="4"/>
<connect gate="G$1" pin="ILIM" pad="8"/>
<connect gate="G$1" pin="SNS" pad="3"/>
<connect gate="G$1" pin="VIN" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DM385" prefix="IC">
<description>&lt;b&gt;DM385_AAR&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: DM385_AAR.bsdl</description>
<gates>
<gate name="G$1" symbol="DM385_AAR"/>
</gates>
<devices>
<device name="" package="AAR">
<connects>
<connect gate="G$1" pin="AUDCLKIN0" pad="AF31"/>
<connect gate="G$1" pin="AUDCLKIN1" pad="AF27"/>
<connect gate="G$1" pin="AUDCLKIN2" pad="AG30"/>
<connect gate="G$1" pin="CLKIN32" pad="AJ31"/>
<connect gate="G$1" pin="CVDD@1" pad="U11"/>
<connect gate="G$1" pin="CVDD@10" pad="P15"/>
<connect gate="G$1" pin="CVDD@11" pad="R15"/>
<connect gate="G$1" pin="CVDD@12" pad="U15"/>
<connect gate="G$1" pin="CVDD@13" pad="V15"/>
<connect gate="G$1" pin="CVDD@14" pad="P17"/>
<connect gate="G$1" pin="CVDD@15" pad="R17"/>
<connect gate="G$1" pin="CVDD@16" pad="T17"/>
<connect gate="G$1" pin="CVDD@17" pad="U17"/>
<connect gate="G$1" pin="CVDD@18" pad="V17"/>
<connect gate="G$1" pin="CVDD@19" pad="T18"/>
<connect gate="G$1" pin="CVDD@2" pad="V11"/>
<connect gate="G$1" pin="CVDD@20" pad="W19"/>
<connect gate="G$1" pin="CVDD@21" pad="Y19"/>
<connect gate="G$1" pin="CVDD@22" pad="W20"/>
<connect gate="G$1" pin="CVDD@23" pad="Y20"/>
<connect gate="G$1" pin="CVDD@3" pad="U12"/>
<connect gate="G$1" pin="CVDD@4" pad="V12"/>
<connect gate="G$1" pin="CVDD@5" pad="T13"/>
<connect gate="G$1" pin="CVDD@6" pad="W13"/>
<connect gate="G$1" pin="CVDD@7" pad="Y13"/>
<connect gate="G$1" pin="CVDD@8" pad="W14"/>
<connect gate="G$1" pin="CVDD@9" pad="Y14"/>
<connect gate="G$1" pin="CVDDARM@1" pad="M13"/>
<connect gate="G$1" pin="CVDDARM@2" pad="M14"/>
<connect gate="G$1" pin="CVDDARM@3" pad="K17"/>
<connect gate="G$1" pin="CVDDARM@4" pad="L17"/>
<connect gate="G$1" pin="CVDDARM@5" pad="M17"/>
<connect gate="G$1" pin="CVDDARM@6" pad="L18"/>
<connect gate="G$1" pin="CVDDHDVICP@1" pad="U20"/>
<connect gate="G$1" pin="CVDDHDVICP@2" pad="V20"/>
<connect gate="G$1" pin="CVDDHDVICP@3" pad="U21"/>
<connect gate="G$1" pin="CVDDHDVICP@4" pad="V21"/>
<connect gate="G$1" pin="CVDDHDVICP@5" pad="W22"/>
<connect gate="G$1" pin="DDR0A0" pad="AL24"/>
<connect gate="G$1" pin="DDR0A1" pad="AC22"/>
<connect gate="G$1" pin="DDR0A10" pad="AD23"/>
<connect gate="G$1" pin="DDR0A11" pad="AK24"/>
<connect gate="G$1" pin="DDR0A12" pad="AH23"/>
<connect gate="G$1" pin="DDR0A13" pad="AK23"/>
<connect gate="G$1" pin="DDR0A14" pad="AL23"/>
<connect gate="G$1" pin="DDR0A15" pad="AK22"/>
<connect gate="G$1" pin="DDR0A2" pad="AJ23"/>
<connect gate="G$1" pin="DDR0A3" pad="AJ27"/>
<connect gate="G$1" pin="DDR0A4" pad="AK28"/>
<connect gate="G$1" pin="DDR0A5" pad="AH27"/>
<connect gate="G$1" pin="DDR0A6" pad="AK30"/>
<connect gate="G$1" pin="DDR0A7" pad="AG23"/>
<connect gate="G$1" pin="DDR0A8" pad="AL29"/>
<connect gate="G$1" pin="DDR0A9" pad="AK29"/>
<connect gate="G$1" pin="DDR0BA0" pad="AK26"/>
<connect gate="G$1" pin="DDR0BA1" pad="AF23"/>
<connect gate="G$1" pin="DDR0BA2" pad="AH25"/>
<connect gate="G$1" pin="DDR0CASN" pad="AK25"/>
<connect gate="G$1" pin="DDR0CKE" pad="AD20"/>
<connect gate="G$1" pin="DDR0CLK" pad="AL27"/>
<connect gate="G$1" pin="DDR0CLKN" pad="AK27"/>
<connect gate="G$1" pin="DDR0CS0N" pad="AB21"/>
<connect gate="G$1" pin="DDR0D0" pad="AL9"/>
<connect gate="G$1" pin="DDR0D1" pad="AK9"/>
<connect gate="G$1" pin="DDR0D10" pad="AD12"/>
<connect gate="G$1" pin="DDR0D11" pad="AB12"/>
<connect gate="G$1" pin="DDR0D12" pad="AK13"/>
<connect gate="G$1" pin="DDR0D13" pad="AC13"/>
<connect gate="G$1" pin="DDR0D14" pad="AL14"/>
<connect gate="G$1" pin="DDR0D15" pad="AK14"/>
<connect gate="G$1" pin="DDR0D16" pad="AH15"/>
<connect gate="G$1" pin="DDR0D17" pad="AF15"/>
<connect gate="G$1" pin="DDR0D18" pad="AD15"/>
<connect gate="G$1" pin="DDR0D19" pad="AK16"/>
<connect gate="G$1" pin="DDR0D2" pad="AK10"/>
<connect gate="G$1" pin="DDR0D20" pad="AJ16"/>
<connect gate="G$1" pin="DDR0D21" pad="AG16"/>
<connect gate="G$1" pin="DDR0D22" pad="AD16"/>
<connect gate="G$1" pin="DDR0D23" pad="AC16"/>
<connect gate="G$1" pin="DDR0D24" pad="AK19"/>
<connect gate="G$1" pin="DDR0D25" pad="AJ19"/>
<connect gate="G$1" pin="DDR0D26" pad="AH19"/>
<connect gate="G$1" pin="DDR0D27" pad="AF19"/>
<connect gate="G$1" pin="DDR0D28" pad="AD19"/>
<connect gate="G$1" pin="DDR0D29" pad="AC19"/>
<connect gate="G$1" pin="DDR0D3" pad="AJ11"/>
<connect gate="G$1" pin="DDR0D30" pad="AJ20"/>
<connect gate="G$1" pin="DDR0D31" pad="AG20"/>
<connect gate="G$1" pin="DDR0D4" pad="AH11"/>
<connect gate="G$1" pin="DDR0D5" pad="AD9"/>
<connect gate="G$1" pin="DDR0D6" pad="AF11"/>
<connect gate="G$1" pin="DDR0D7" pad="AL12"/>
<connect gate="G$1" pin="DDR0D8" pad="AJ12"/>
<connect gate="G$1" pin="DDR0D9" pad="AG12"/>
<connect gate="G$1" pin="DDR0DQM0" pad="AL8"/>
<connect gate="G$1" pin="DDR0DQM1" pad="AK12"/>
<connect gate="G$1" pin="DDR0DQM2" pad="AJ15"/>
<connect gate="G$1" pin="DDR0DQM3" pad="AK18"/>
<connect gate="G$1" pin="DDR0DQS0" pad="AL11"/>
<connect gate="G$1" pin="DDR0DQS0N" pad="AK11"/>
<connect gate="G$1" pin="DDR0DQS1" pad="AL15"/>
<connect gate="G$1" pin="DDR0DQS1N" pad="AK15"/>
<connect gate="G$1" pin="DDR0DQS2" pad="AL17"/>
<connect gate="G$1" pin="DDR0DQS2N" pad="AK17"/>
<connect gate="G$1" pin="DDR0DQS3" pad="AL20"/>
<connect gate="G$1" pin="DDR0DQS3N" pad="AK20"/>
<connect gate="G$1" pin="DDR0ODT0" pad="AL21"/>
<connect gate="G$1" pin="DDR0RASN" pad="AJ25"/>
<connect gate="G$1" pin="DDR0RST" pad="AA20"/>
<connect gate="G$1" pin="DDR0WEN" pad="AL26"/>
<connect gate="G$1" pin="DEVOSCWAKE" pad="U28"/>
<connect gate="G$1" pin="DVDD@1" pad="M4"/>
<connect gate="G$1" pin="DVDD@10" pad="T26"/>
<connect gate="G$1" pin="DVDD@11" pad="U27"/>
<connect gate="G$1" pin="DVDD@12" pad="T28"/>
<connect gate="G$1" pin="DVDD@2" pad="L5"/>
<connect gate="G$1" pin="DVDD@3" pad="M6"/>
<connect gate="G$1" pin="DVDD@4" pad="M7"/>
<connect gate="G$1" pin="DVDD@5" pad="N10"/>
<connect gate="G$1" pin="DVDD@6" pad="N11"/>
<connect gate="G$1" pin="DVDD@7" pad="D16"/>
<connect gate="G$1" pin="DVDD@8" pad="F16"/>
<connect gate="G$1" pin="DVDD@9" pad="E17"/>
<connect gate="G$1" pin="DVDDC@1" pad="D12"/>
<connect gate="G$1" pin="DVDDC@2" pad="F12"/>
<connect gate="G$1" pin="DVDDC@3" pad="G12"/>
<connect gate="G$1" pin="DVDDC@4" pad="E13"/>
<connect gate="G$1" pin="DVDDC@5" pad="G13"/>
<connect gate="G$1" pin="DVDDDDR0@1" pad="AB14"/>
<connect gate="G$1" pin="DVDDDDR0@10" pad="AC17"/>
<connect gate="G$1" pin="DVDDDDR0@11" pad="AB18"/>
<connect gate="G$1" pin="DVDDDDR0@12" pad="AC18"/>
<connect gate="G$1" pin="DVDDDDR0@2" pad="AB15"/>
<connect gate="G$1" pin="DVDDDDR0@3" pad="AC15"/>
<connect gate="G$1" pin="DVDDDDR0@4" pad="AE15"/>
<connect gate="G$1" pin="DVDDDDR0@5" pad="AG15"/>
<connect gate="G$1" pin="DVDDDDR0@6" pad="AE16"/>
<connect gate="G$1" pin="DVDDDDR0@7" pad="AF16"/>
<connect gate="G$1" pin="DVDDDDR0@8" pad="AH16"/>
<connect gate="G$1" pin="DVDDDDR0@9" pad="AB17"/>
<connect gate="G$1" pin="DVDDGPMC@1" pad="T4"/>
<connect gate="G$1" pin="DVDDGPMC@2" pad="R5"/>
<connect gate="G$1" pin="DVDDGPMC@3" pad="T6"/>
<connect gate="G$1" pin="DVDDGPMC@4" pad="R7"/>
<connect gate="G$1" pin="DVDDGPMC@5" pad="T7"/>
<connect gate="G$1" pin="DVDDRGMII@1" pad="Y4"/>
<connect gate="G$1" pin="DVDDRGMII@2" pad="W5"/>
<connect gate="G$1" pin="DVDDRGMII@3" pad="Y6"/>
<connect gate="G$1" pin="DVDDRGMII@4" pad="W7"/>
<connect gate="G$1" pin="DVDDRGMII@5" pad="Y7"/>
<connect gate="G$1" pin="DVDDSD@1" pad="T25"/>
<connect gate="G$1" pin="DVDDSD@2" pad="U25"/>
<connect gate="G$1" pin="EMAC0GMTCLK_EMAC1RGRXC" pad="AL6"/>
<connect gate="G$1" pin="EMAC0MCOL_EMAC0RGRXCTL" pad="AH1"/>
<connect gate="G$1" pin="EMAC0MCRS_EMAC0RGRXD2" pad="AH2"/>
<connect gate="G$1" pin="EMAC0MRCLK_EMAC0RGTXC" pad="AK1"/>
<connect gate="G$1" pin="EMAC0MRXD0_EMAC0RGTXD0" pad="AK2"/>
<connect gate="G$1" pin="EMAC0MRXD1_EMAC0RGRXD0" pad="AL2"/>
<connect gate="G$1" pin="EMAC0MRXD2_EMAC0RGRXD1" pad="AL3"/>
<connect gate="G$1" pin="EMAC0MRXD3_EMAC1RGRXCTL" pad="AK3"/>
<connect gate="G$1" pin="EMAC0MRXD4_EMAC0RGRXD3" pad="AK4"/>
<connect gate="G$1" pin="EMAC0MRXD5_EMAC0RGTXD3" pad="AJ4"/>
<connect gate="G$1" pin="EMAC0MRXD6_EMAC0RGTXD2" pad="AL5"/>
<connect gate="G$1" pin="EMAC0MRXD7_EMAC0RGTXD1" pad="AK5"/>
<connect gate="G$1" pin="EMAC0MRXDV_EMAC1RGRXD1" pad="AJ6"/>
<connect gate="G$1" pin="EMAC0MRXER_EMAC0RGTXCTL" pad="AJ2"/>
<connect gate="G$1" pin="EMAC0MTCLK_EMAC0RGRXC" pad="AG4"/>
<connect gate="G$1" pin="EMAC0MTXD0_EMAC1RGRXD3" pad="AK6"/>
<connect gate="G$1" pin="EMAC0MTXD1_EMAC1RGTXD1" pad="AJ7"/>
<connect gate="G$1" pin="EMAC0MTXD2_EMAC1RGTXCTL" pad="AK7"/>
<connect gate="G$1" pin="EMAC0MTXD3_EMAC1RGTXD0" pad="AE4"/>
<connect gate="G$1" pin="EMAC0MTXD4_EMAC1RGTXD2" pad="AK8"/>
<connect gate="G$1" pin="EMAC0MTXD5_EMAC1RGTXC" pad="AJ8"/>
<connect gate="G$1" pin="EMAC0MTXD6_EMAC1RGRXD0" pad="AH8"/>
<connect gate="G$1" pin="EMAC0MTXD7_EMAC1RGTXD3" pad="AG8"/>
<connect gate="G$1" pin="EMAC0MTXEN_EMAC1RGRXD2" pad="AF8"/>
<connect gate="G$1" pin="EMACRMREFCLK" pad="AG1"/>
<connect gate="G$1" pin="EMU0" pad="A18"/>
<connect gate="G$1" pin="EMU1" pad="B19"/>
<connect gate="G$1" pin="GPMCA16" pad="M1"/>
<connect gate="G$1" pin="GPMCA17" pad="M2"/>
<connect gate="G$1" pin="GPMCA18" pad="M3"/>
<connect gate="G$1" pin="GPMCA19" pad="M5"/>
<connect gate="G$1" pin="GPMCA20" pad="N9"/>
<connect gate="G$1" pin="GPMCA21" pad="N1"/>
<connect gate="G$1" pin="GPMCA22" pad="N2"/>
<connect gate="G$1" pin="GPMCA23" pad="R8"/>
<connect gate="G$1" pin="GPMCADVNALE" pad="AA10"/>
<connect gate="G$1" pin="GPMCBE0NCLE" pad="Y3"/>
<connect gate="G$1" pin="GPMCBE1N" pad="Y11"/>
<connect gate="G$1" pin="GPMCCLK" pad="AB9"/>
<connect gate="G$1" pin="GPMCCS0N" pad="AC9"/>
<connect gate="G$1" pin="GPMCCS1N" pad="AA12"/>
<connect gate="G$1" pin="GPMCCS2N" pad="AC3"/>
<connect gate="G$1" pin="GPMCCS3N" pad="AF2"/>
<connect gate="G$1" pin="GPMCCS4N" pad="AG6"/>
<connect gate="G$1" pin="GPMCD0" pad="W6"/>
<connect gate="G$1" pin="GPMCD1" pad="W4"/>
<connect gate="G$1" pin="GPMCD10" pad="R6"/>
<connect gate="G$1" pin="GPMCD11" pad="R4"/>
<connect gate="G$1" pin="GPMCD12" pad="R3"/>
<connect gate="G$1" pin="GPMCD13" pad="R2"/>
<connect gate="G$1" pin="GPMCD14" pad="R1"/>
<connect gate="G$1" pin="GPMCD15" pad="P2"/>
<connect gate="G$1" pin="GPMCD2" pad="W3"/>
<connect gate="G$1" pin="GPMCD3" pad="U2"/>
<connect gate="G$1" pin="GPMCD4" pad="W9"/>
<connect gate="G$1" pin="GPMCD5" pad="T5"/>
<connect gate="G$1" pin="GPMCD6" pad="T3"/>
<connect gate="G$1" pin="GPMCD7" pad="T2"/>
<connect gate="G$1" pin="GPMCD8" pad="T1"/>
<connect gate="G$1" pin="GPMCD9" pad="T8"/>
<connect gate="G$1" pin="GPMCOEREN" pad="Y8"/>
<connect gate="G$1" pin="GPMCWAIT0" pad="W8"/>
<connect gate="G$1" pin="GPMCWEN" pad="Y5"/>
<connect gate="G$1" pin="HDDACHSYNC" pad="E9"/>
<connect gate="G$1" pin="HDDACVSYNC" pad="D9"/>
<connect gate="G$1" pin="I2C0SCL" pad="T27"/>
<connect gate="G$1" pin="I2C0SDA" pad="T24"/>
<connect gate="G$1" pin="I2C1SCL" pad="D2"/>
<connect gate="G$1" pin="I2C1SDA" pad="D1"/>
<connect gate="G$1" pin="LDOCAPARM" pad="J19"/>
<connect gate="G$1" pin="LDOCAPARMRAM" pad="K20"/>
<connect gate="G$1" pin="LDOCAPHDVICP" pad="W23"/>
<connect gate="G$1" pin="LDOCAPHDVICPRAM" pad="Y24"/>
<connect gate="G$1" pin="LDOCAPRAM0" pad="U9"/>
<connect gate="G$1" pin="LDOCAPRAM1" pad="T22"/>
<connect gate="G$1" pin="LDOCAPRAM2" pad="AB10"/>
<connect gate="G$1" pin="LDOCAPSERDESCLK" pad="M24"/>
<connect gate="G$1" pin="MCA0ACLKR" pad="AD30"/>
<connect gate="G$1" pin="MCA0ACLKX" pad="AD28"/>
<connect gate="G$1" pin="MCA0AFSR" pad="AF30"/>
<connect gate="G$1" pin="MCA0AFSX" pad="AE29"/>
<connect gate="G$1" pin="MCA0AXR0" pad="AF29"/>
<connect gate="G$1" pin="MCA0AXR1" pad="AE31"/>
<connect gate="G$1" pin="MCA0AXR2" pad="AE30"/>
<connect gate="G$1" pin="MCA0AXR3" pad="AC31"/>
<connect gate="G$1" pin="MCA0AXR4" pad="AD26"/>
<connect gate="G$1" pin="MCA0AXR5" pad="AD27"/>
<connect gate="G$1" pin="MCA1ACLKR" pad="AD29"/>
<connect gate="G$1" pin="MCA1ACLKX" pad="AC23"/>
<connect gate="G$1" pin="MCA1AFSR" pad="AC24"/>
<connect gate="G$1" pin="MCA1AFSX" pad="AB22"/>
<connect gate="G$1" pin="MCA1AXR0" pad="Y22"/>
<connect gate="G$1" pin="MCA1AXR1" pad="Y21"/>
<connect gate="G$1" pin="MDCLK" pad="AG2"/>
<connect gate="G$1" pin="MDIO" pad="AG3"/>
<connect gate="G$1" pin="NMIN" pad="AH31"/>
<connect gate="G$1" pin="PORN" pad="AH30"/>
<connect gate="G$1" pin="RESETN" pad="AH29"/>
<connect gate="G$1" pin="RSTOUTWDOUTN" pad="AJ30"/>
<connect gate="G$1" pin="RSV4" pad="G17"/>
<connect gate="G$1" pin="RSV42" pad="AK21"/>
<connect gate="G$1" pin="RSV5" pad="G16"/>
<connect gate="G$1" pin="RSV54" pad="M28"/>
<connect gate="G$1" pin="RSV55" pad="N27"/>
<connect gate="G$1" pin="SD0CLK" pad="AB30"/>
<connect gate="G$1" pin="SD0CMD" pad="AA29"/>
<connect gate="G$1" pin="SD0DAT0" pad="AA28"/>
<connect gate="G$1" pin="SD0DAT1SDIRQN" pad="AA26"/>
<connect gate="G$1" pin="SD0DAT2SDRWN" pad="Y31"/>
<connect gate="G$1" pin="SD0DAT3" pad="Y30"/>
<connect gate="G$1" pin="SD0DAT6" pad="AB31"/>
<connect gate="G$1" pin="SD0DAT7" pad="AC30"/>
<connect gate="G$1" pin="SD1CLK" pad="W30"/>
<connect gate="G$1" pin="SD1CMD" pad="Y29"/>
<connect gate="G$1" pin="SD1DAT0" pad="W31"/>
<connect gate="G$1" pin="SD1DAT1SDIRQN" pad="AA30"/>
<connect gate="G$1" pin="SD1DAT2SDRWN" pad="U29"/>
<connect gate="G$1" pin="SD1DAT3" pad="Y27"/>
<connect gate="G$1" pin="SD2DAT0" pad="AC4"/>
<connect gate="G$1" pin="SD2DAT1SDIRQN" pad="AC5"/>
<connect gate="G$1" pin="SD2DAT2SDRWN" pad="AC8"/>
<connect gate="G$1" pin="SD2DAT3" pad="AD1"/>
<connect gate="G$1" pin="SD2DAT4" pad="AD2"/>
<connect gate="G$1" pin="SD2DAT5" pad="AE1"/>
<connect gate="G$1" pin="SD2DAT6" pad="AE2"/>
<connect gate="G$1" pin="SD2DAT7" pad="AE3"/>
<connect gate="G$1" pin="SD2SCLK" pad="AC6"/>
<connect gate="G$1" pin="SPI0D0" pad="J28"/>
<connect gate="G$1" pin="SPI0D1" pad="J27"/>
<connect gate="G$1" pin="SPI0SCLK" pad="N24"/>
<connect gate="G$1" pin="SPI0SCS0N" pad="G29"/>
<connect gate="G$1" pin="SPI0SCS1N" pad="G28"/>
<connect gate="G$1" pin="SPI1D0" pad="N23"/>
<connect gate="G$1" pin="SPI1D1" pad="M27"/>
<connect gate="G$1" pin="SPI1SCLK" pad="M29"/>
<connect gate="G$1" pin="SPI1SCS0N" pad="J29"/>
<connect gate="G$1" pin="TCLK" pad="T29"/>
<connect gate="G$1" pin="TDI" pad="N28"/>
<connect gate="G$1" pin="TDO" pad="U26"/>
<connect gate="G$1" pin="TMS" pad="T31"/>
<connect gate="G$1" pin="TRSTN" pad="U24"/>
<connect gate="G$1" pin="UART0CTSN" pad="D30"/>
<connect gate="G$1" pin="UART0DCDN" pad="E31"/>
<connect gate="G$1" pin="UART0DSRN" pad="E29"/>
<connect gate="G$1" pin="UART0DTRN" pad="E30"/>
<connect gate="G$1" pin="UART0RIN" pad="N26"/>
<connect gate="G$1" pin="UART0RTSN" pad="D31"/>
<connect gate="G$1" pin="UART0RXD" pad="J26"/>
<connect gate="G$1" pin="UART0TXD" pad="E28"/>
<connect gate="G$1" pin="UART2RXD" pad="L22"/>
<connect gate="G$1" pin="UART2TXD" pad="M21"/>
<connect gate="G$1" pin="USB0DRVVBUS" pad="K23"/>
<connect gate="G$1" pin="VDDA1P8@1" pad="R9"/>
<connect gate="G$1" pin="VDDA1P8@2" pad="T9"/>
<connect gate="G$1" pin="VDDA1P8@3" pad="T10"/>
<connect gate="G$1" pin="VDDA1P8@4" pad="N22"/>
<connect gate="G$1" pin="VDDA1P8@5" pad="P23"/>
<connect gate="G$1" pin="VDDA1P8@6" pad="M25"/>
<connect gate="G$1" pin="VDDA1P8@7" pad="N25"/>
<connect gate="G$1" pin="VDDAARMPLL1P8" pad="L19"/>
<connect gate="G$1" pin="VDDAAUDIOPLL1P8" pad="V9"/>
<connect gate="G$1" pin="VDDACSI21P8" pad="W10"/>
<connect gate="G$1" pin="VDDADDRPLL1P8" pad="AA19"/>
<connect gate="G$1" pin="VDDAHDDAC1P1" pad="K16"/>
<connect gate="G$1" pin="VDDAHDDAC1P8" pad="L14"/>
<connect gate="G$1" pin="VDDAHDDACREF1P8" pad="L15"/>
<connect gate="G$1" pin="VDDAHDMI1P8" pad="K14"/>
<connect gate="G$1" pin="VDDAHDVICPPLL1P8" pad="T23"/>
<connect gate="G$1" pin="VDDAL3L41P8" pad="W11"/>
<connect gate="G$1" pin="VDDAPCIE1P8" pad="M26"/>
<connect gate="G$1" pin="VDDAUSB01P8" pad="K19"/>
<connect gate="G$1" pin="VDDAUSB11P8" pad="J17"/>
<connect gate="G$1" pin="VDDAUSB3P3@1" pad="M19"/>
<connect gate="G$1" pin="VDDAUSB3P3@2" pad="M20"/>
<connect gate="G$1" pin="VDDAVDAC1P8" pad="J14"/>
<connect gate="G$1" pin="VDDAVIDPLL1P8" pad="L13"/>
<connect gate="G$1" pin="VDDSOSC01P8" pad="P21"/>
<connect gate="G$1" pin="VDDSOSC11P8" pad="P20"/>
<connect gate="G$1" pin="VIN0ACLK" pad="C9"/>
<connect gate="G$1" pin="VIN0AD0" pad="B18"/>
<connect gate="G$1" pin="VIN0AD1" pad="A17"/>
<connect gate="G$1" pin="VIN0AD10BD2" pad="E16"/>
<connect gate="G$1" pin="VIN0AD11BD3" pad="H17"/>
<connect gate="G$1" pin="VIN0AD12BD4" pad="J16"/>
<connect gate="G$1" pin="VIN0AD13BD5" pad="H16"/>
<connect gate="G$1" pin="VIN0AD14BD6" pad="F13"/>
<connect gate="G$1" pin="VIN0AD15BD7" pad="H13"/>
<connect gate="G$1" pin="VIN0AD16" pad="K11"/>
<connect gate="G$1" pin="VIN0AD17" pad="E12"/>
<connect gate="G$1" pin="VIN0AD18" pad="K10"/>
<connect gate="G$1" pin="VIN0AD19" pad="D7"/>
<connect gate="G$1" pin="VIN0AD2" pad="B17"/>
<connect gate="G$1" pin="VIN0AD20" pad="F9"/>
<connect gate="G$1" pin="VIN0AD21" pad="C7"/>
<connect gate="G$1" pin="VIN0AD22" pad="A6"/>
<connect gate="G$1" pin="VIN0AD23" pad="A5"/>
<connect gate="G$1" pin="VIN0AD3" pad="C17"/>
<connect gate="G$1" pin="VIN0AD4" pad="D17"/>
<connect gate="G$1" pin="VIN0AD5" pad="F17"/>
<connect gate="G$1" pin="VIN0AD6" pad="L20"/>
<connect gate="G$1" pin="VIN0AD7" pad="H20"/>
<connect gate="G$1" pin="VIN0AD8BD0" pad="B16"/>
<connect gate="G$1" pin="VIN0AD9BD1" pad="C16"/>
<connect gate="G$1" pin="VIN0ADE" pad="C12"/>
<connect gate="G$1" pin="VIN0ADE1" pad="B5"/>
<connect gate="G$1" pin="VIN0AFLD" pad="J13"/>
<connect gate="G$1" pin="VIN0AFLD1" pad="B4"/>
<connect gate="G$1" pin="VIN0AHSYNC" pad="D13"/>
<connect gate="G$1" pin="VIN0AVSYNC" pad="C13"/>
<connect gate="G$1" pin="VIN0BCLK" pad="H12"/>
<connect gate="G$1" pin="VIN0BDE" pad="C5"/>
<connect gate="G$1" pin="VIN0BFLD" pad="A3"/>
<connect gate="G$1" pin="VOUT0AVID" pad="C20"/>
<connect gate="G$1" pin="VOUT0BCBC2" pad="F24"/>
<connect gate="G$1" pin="VOUT0BCBC3" pad="D21"/>
<connect gate="G$1" pin="VOUT0BCBC4" pad="J23"/>
<connect gate="G$1" pin="VOUT0BCBC5" pad="H23"/>
<connect gate="G$1" pin="VOUT0BCBC6" pad="J24"/>
<connect gate="G$1" pin="VOUT0BCBC7" pad="E24"/>
<connect gate="G$1" pin="VOUT0BCBC8" pad="D24"/>
<connect gate="G$1" pin="VOUT0BCBC9" pad="C24"/>
<connect gate="G$1" pin="VOUT0CLK" pad="K22"/>
<connect gate="G$1" pin="VOUT0FLD" pad="B3"/>
<connect gate="G$1" pin="VOUT0GYYC2" pad="C25"/>
<connect gate="G$1" pin="VOUT0GYYC3" pad="C26"/>
<connect gate="G$1" pin="VOUT0GYYC4" pad="E26"/>
<connect gate="G$1" pin="VOUT0GYYC5" pad="B26"/>
<connect gate="G$1" pin="VOUT0GYYC6" pad="A26"/>
<connect gate="G$1" pin="VOUT0GYYC7" pad="B25"/>
<connect gate="G$1" pin="VOUT0GYYC8" pad="B27"/>
<connect gate="G$1" pin="VOUT0GYYC9" pad="A27"/>
<connect gate="G$1" pin="VOUT0HSYNC" pad="F21"/>
<connect gate="G$1" pin="VOUT0RCR2" pad="C28"/>
<connect gate="G$1" pin="VOUT0RCR3" pad="B28"/>
<connect gate="G$1" pin="VOUT0RCR4" pad="B29"/>
<connect gate="G$1" pin="VOUT0RCR5" pad="A29"/>
<connect gate="G$1" pin="VOUT0RCR6" pad="C30"/>
<connect gate="G$1" pin="VOUT0RCR7" pad="B30"/>
<connect gate="G$1" pin="VOUT0RCR8" pad="A30"/>
<connect gate="G$1" pin="VOUT0RCR9" pad="B31"/>
<connect gate="G$1" pin="VOUT0VSYNC" pad="E20"/>
<connect gate="G$1" pin="VOUT1AVID" pad="F1"/>
<connect gate="G$1" pin="VOUT1BCBC0" pad="H9"/>
<connect gate="G$1" pin="VOUT1BCBC1" pad="D5"/>
<connect gate="G$1" pin="VOUT1BCBC2" pad="M8"/>
<connect gate="G$1" pin="VOUT1BCBC3" pad="F2"/>
<connect gate="G$1" pin="VOUT1BCBC4" pad="F3"/>
<connect gate="G$1" pin="VOUT1BCBC5" pad="G1"/>
<connect gate="G$1" pin="VOUT1BCBC6" pad="G2"/>
<connect gate="G$1" pin="VOUT1BCBC7" pad="H3"/>
<connect gate="G$1" pin="VOUT1BCBC8" pad="G3"/>
<connect gate="G$1" pin="VOUT1BCBC9" pad="H5"/>
<connect gate="G$1" pin="VOUT1CLK" pad="D3"/>
<connect gate="G$1" pin="VOUT1FLD" pad="J10"/>
<connect gate="G$1" pin="VOUT1GYYC0" pad="B2"/>
<connect gate="G$1" pin="VOUT1GYYC1" pad="A2"/>
<connect gate="G$1" pin="VOUT1GYYC2" pad="L2"/>
<connect gate="G$1" pin="VOUT1GYYC3" pad="H6"/>
<connect gate="G$1" pin="VOUT1GYYC4" pad="J8"/>
<connect gate="G$1" pin="VOUT1GYYC5" pad="J1"/>
<connect gate="G$1" pin="VOUT1GYYC6" pad="H4"/>
<connect gate="G$1" pin="VOUT1GYYC7" pad="J9"/>
<connect gate="G$1" pin="VOUT1GYYC8" pad="L3"/>
<connect gate="G$1" pin="VOUT1GYYC9" pad="K1"/>
<connect gate="G$1" pin="VOUT1HSYNC" pad="E2"/>
<connect gate="G$1" pin="VOUT1RCR0" pad="C2"/>
<connect gate="G$1" pin="VOUT1RCR1" pad="C1"/>
<connect gate="G$1" pin="VOUT1RCR2" pad="L6"/>
<connect gate="G$1" pin="VOUT1RCR3" pad="L4"/>
<connect gate="G$1" pin="VOUT1RCR4" pad="H2"/>
<connect gate="G$1" pin="VOUT1RCR5" pad="M11"/>
<connect gate="G$1" pin="VOUT1RCR6" pad="L12"/>
<connect gate="G$1" pin="VOUT1RCR7" pad="M10"/>
<connect gate="G$1" pin="VOUT1RCR8" pad="J2"/>
<connect gate="G$1" pin="VOUT1RCR9" pad="K2"/>
<connect gate="G$1" pin="VOUT1VSYNC" pad="F5"/>
<connect gate="G$1" pin="VREFSSTLDDR0" pad="AL18"/>
<connect gate="G$1" pin="VSS@1" pad="A1"/>
<connect gate="G$1" pin="VSS@10" pad="AD6"/>
<connect gate="G$1" pin="VSS@100" pad="AA27"/>
<connect gate="G$1" pin="VSS@101" pad="AE27"/>
<connect gate="G$1" pin="VSS@102" pad="Y28"/>
<connect gate="G$1" pin="VSS@103" pad="AE28"/>
<connect gate="G$1" pin="VSS@104" pad="A31"/>
<connect gate="G$1" pin="VSS@105" pad="AL31"/>
<connect gate="G$1" pin="VSS@11" pad="AE6"/>
<connect gate="G$1" pin="VSS@12" pad="E7"/>
<connect gate="G$1" pin="VSS@13" pad="F7"/>
<connect gate="G$1" pin="VSS@14" pad="G7"/>
<connect gate="G$1" pin="VSS@15" pad="H7"/>
<connect gate="G$1" pin="VSS@16" pad="J7"/>
<connect gate="G$1" pin="VSS@17" pad="AD7"/>
<connect gate="G$1" pin="VSS@18" pad="AE7"/>
<connect gate="G$1" pin="VSS@19" pad="AF7"/>
<connect gate="G$1" pin="VSS@2" pad="AL1"/>
<connect gate="G$1" pin="VSS@20" pad="AG7"/>
<connect gate="G$1" pin="VSS@21" pad="AH7"/>
<connect gate="G$1" pin="VSS@22" pad="D8"/>
<connect gate="G$1" pin="VSS@23" pad="E8"/>
<connect gate="G$1" pin="VSS@24" pad="F8"/>
<connect gate="G$1" pin="VSS@25" pad="G8"/>
<connect gate="G$1" pin="VSS@26" pad="AE8"/>
<connect gate="G$1" pin="VSS@27" pad="AE9"/>
<connect gate="G$1" pin="VSS@28" pad="P11"/>
<connect gate="G$1" pin="VSS@29" pad="R11"/>
<connect gate="G$1" pin="VSS@3" pad="AD3"/>
<connect gate="G$1" pin="VSS@30" pad="T11"/>
<connect gate="G$1" pin="VSS@31" pad="AG11"/>
<connect gate="G$1" pin="VSS@32" pad="P12"/>
<connect gate="G$1" pin="VSS@33" pad="R12"/>
<connect gate="G$1" pin="VSS@34" pad="T12"/>
<connect gate="G$1" pin="VSS@35" pad="AE12"/>
<connect gate="G$1" pin="VSS@36" pad="AF12"/>
<connect gate="G$1" pin="VSS@37" pad="AH12"/>
<connect gate="G$1" pin="VSS@38" pad="N13"/>
<connect gate="G$1" pin="VSS@39" pad="AA13"/>
<connect gate="G$1" pin="VSS@4" pad="G4"/>
<connect gate="G$1" pin="VSS@40" pad="N14"/>
<connect gate="G$1" pin="VSS@41" pad="P14"/>
<connect gate="G$1" pin="VSS@42" pad="R14"/>
<connect gate="G$1" pin="VSS@43" pad="T14"/>
<connect gate="G$1" pin="VSS@44" pad="U14"/>
<connect gate="G$1" pin="VSS@45" pad="AA14"/>
<connect gate="G$1" pin="VSS@46" pad="T15"/>
<connect gate="G$1" pin="VSS@47" pad="AA15"/>
<connect gate="G$1" pin="VSS@48" pad="L16"/>
<connect gate="G$1" pin="VSS@49" pad="M16"/>
<connect gate="G$1" pin="VSS@5" pad="AD4"/>
<connect gate="G$1" pin="VSS@50" pad="N16"/>
<connect gate="G$1" pin="VSS@51" pad="T16"/>
<connect gate="G$1" pin="VSS@52" pad="W16"/>
<connect gate="G$1" pin="VSS@53" pad="Y16"/>
<connect gate="G$1" pin="VSS@54" pad="AA16"/>
<connect gate="G$1" pin="VSS@55" pad="N17"/>
<connect gate="G$1" pin="VSS@56" pad="W17"/>
<connect gate="G$1" pin="VSS@57" pad="Y17"/>
<connect gate="G$1" pin="VSS@58" pad="AA17"/>
<connect gate="G$1" pin="VSS@59" pad="P18"/>
<connect gate="G$1" pin="VSS@6" pad="G5"/>
<connect gate="G$1" pin="VSS@60" pad="R18"/>
<connect gate="G$1" pin="VSS@61" pad="U18"/>
<connect gate="G$1" pin="VSS@62" pad="V18"/>
<connect gate="G$1" pin="VSS@63" pad="AA18"/>
<connect gate="G$1" pin="VSS@64" pad="T19"/>
<connect gate="G$1" pin="VSS@65" pad="AE19"/>
<connect gate="G$1" pin="VSS@66" pad="AG19"/>
<connect gate="G$1" pin="VSS@67" pad="F20"/>
<connect gate="G$1" pin="VSS@68" pad="G20"/>
<connect gate="G$1" pin="VSS@69" pad="R20"/>
<connect gate="G$1" pin="VSS@7" pad="AD5"/>
<connect gate="G$1" pin="VSS@70" pad="T20"/>
<connect gate="G$1" pin="VSS@71" pad="AE20"/>
<connect gate="G$1" pin="VSS@72" pad="AF20"/>
<connect gate="G$1" pin="VSS@73" pad="AH20"/>
<connect gate="G$1" pin="VSS@74" pad="E21"/>
<connect gate="G$1" pin="VSS@75" pad="R21"/>
<connect gate="G$1" pin="VSS@76" pad="T21"/>
<connect gate="G$1" pin="VSS@77" pad="G23"/>
<connect gate="G$1" pin="VSS@78" pad="U23"/>
<connect gate="G$1" pin="VSS@79" pad="AE23"/>
<connect gate="G$1" pin="VSS@8" pad="AE5"/>
<connect gate="G$1" pin="VSS@80" pad="G24"/>
<connect gate="G$1" pin="VSS@81" pad="AD24"/>
<connect gate="G$1" pin="VSS@82" pad="AE24"/>
<connect gate="G$1" pin="VSS@83" pad="AF24"/>
<connect gate="G$1" pin="VSS@84" pad="AG24"/>
<connect gate="G$1" pin="VSS@85" pad="D25"/>
<connect gate="G$1" pin="VSS@86" pad="E25"/>
<connect gate="G$1" pin="VSS@87" pad="F25"/>
<connect gate="G$1" pin="VSS@88" pad="G25"/>
<connect gate="G$1" pin="VSS@89" pad="Y25"/>
<connect gate="G$1" pin="VSS@9" pad="G6"/>
<connect gate="G$1" pin="VSS@90" pad="AC25"/>
<connect gate="G$1" pin="VSS@91" pad="AD25"/>
<connect gate="G$1" pin="VSS@92" pad="AE25"/>
<connect gate="G$1" pin="VSS@93" pad="AF25"/>
<connect gate="G$1" pin="VSS@94" pad="AG25"/>
<connect gate="G$1" pin="VSS@95" pad="G26"/>
<connect gate="G$1" pin="VSS@96" pad="H26"/>
<connect gate="G$1" pin="VSS@97" pad="Y26"/>
<connect gate="G$1" pin="VSS@98" pad="AE26"/>
<connect gate="G$1" pin="VSS@99" pad="G27"/>
<connect gate="G$1" pin="VSSAAUXOSC" pad="U30"/>
<connect gate="G$1" pin="VSSACSI2@1" pad="AC7"/>
<connect gate="G$1" pin="VSSACSI2@2" pad="V14"/>
<connect gate="G$1" pin="VSSADEVOSC" pad="G30"/>
<connect gate="G$1" pin="VSSAHDMI@1" pad="H8"/>
<connect gate="G$1" pin="VSSAHDMI@2" pad="G9"/>
<connect gate="G$1" pin="VSSAUSB@1" pad="N19"/>
<connect gate="G$1" pin="VSSAUSB@2" pad="D20"/>
<connect gate="G$1" pin="VSSAUSB@3" pad="N20"/>
<connect gate="G$1" pin="VSSAVDAC" pad="C8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DM385_DAVINCI" prefix="IC">
<description>&lt;b&gt;DM385_AAR&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: DM385_AAR.bsdl&lt;br&gt;&lt;i&gt;Connect-List generated from &lt;/i&gt;&lt;b&gt;DM385.DEV&lt;/b&gt; Variant &lt;b&gt;''&lt;/b&gt; with &lt;i&gt;&lt;b&gt;connect-device-split-symbol.ulp&lt;/b&gt;&lt;/i&gt;</description>
<gates>
<gate name="A" symbol="DM385_A"/>
<gate name="B" symbol="DM385_DDR"/>
<gate name="C" symbol="DM385_EMA"/>
<gate name="D" symbol="DM385_GPM"/>
<gate name="E" symbol="DM385_MCA"/>
<gate name="F" symbol="DM385_SD"/>
<gate name="G" symbol="DM385_SPI"/>
<gate name="H" symbol="DM385_UART"/>
<gate name="I" symbol="DM385_I2C"/>
<gate name="K" symbol="DM385_VIN"/>
<gate name="L" symbol="DM385_VOUT"/>
<gate name="M" symbol="DM385_CVDD"/>
<gate name="N" symbol="DM385_DVDD"/>
<gate name="O" symbol="DM385_VDD"/>
<gate name="P" symbol="DM385_VSS"/>
<gate name="Q" symbol="DM385_RSV"/>
<gate name="J" symbol="DM385_LDO"/>
</gates>
<devices>
<device name="" package="AAR">
<connects>
<connect gate="A" pin="AUDCLKIN0" pad="AF31"/>
<connect gate="A" pin="AUDCLKIN1" pad="AF27"/>
<connect gate="A" pin="AUDCLKIN2" pad="AG30"/>
<connect gate="A" pin="CLKIN32" pad="AJ31"/>
<connect gate="A" pin="DEVOSCWAKE" pad="U28"/>
<connect gate="A" pin="EMU0" pad="A18"/>
<connect gate="A" pin="EMU1" pad="B19"/>
<connect gate="A" pin="HDDACHSYNC" pad="E9"/>
<connect gate="A" pin="HDDACVSYNC" pad="D9"/>
<connect gate="A" pin="MDCLK" pad="AG2"/>
<connect gate="A" pin="MDIO" pad="AG3"/>
<connect gate="A" pin="NMIN" pad="AH31"/>
<connect gate="A" pin="PORN" pad="AH30"/>
<connect gate="A" pin="RESETN" pad="AH29"/>
<connect gate="A" pin="RSTOUTWDOUTN" pad="AJ30"/>
<connect gate="A" pin="TCLK" pad="T29"/>
<connect gate="A" pin="TDI" pad="N28"/>
<connect gate="A" pin="TDO" pad="U26"/>
<connect gate="A" pin="TMS" pad="T31"/>
<connect gate="A" pin="TRSTN" pad="U24"/>
<connect gate="B" pin="DDR0A0" pad="AL24"/>
<connect gate="B" pin="DDR0A1" pad="AC22"/>
<connect gate="B" pin="DDR0A10" pad="AD23"/>
<connect gate="B" pin="DDR0A11" pad="AK24"/>
<connect gate="B" pin="DDR0A12" pad="AH23"/>
<connect gate="B" pin="DDR0A13" pad="AK23"/>
<connect gate="B" pin="DDR0A14" pad="AL23"/>
<connect gate="B" pin="DDR0A15" pad="AK22"/>
<connect gate="B" pin="DDR0A2" pad="AJ23"/>
<connect gate="B" pin="DDR0A3" pad="AJ27"/>
<connect gate="B" pin="DDR0A4" pad="AK28"/>
<connect gate="B" pin="DDR0A5" pad="AH27"/>
<connect gate="B" pin="DDR0A6" pad="AK30"/>
<connect gate="B" pin="DDR0A7" pad="AG23"/>
<connect gate="B" pin="DDR0A8" pad="AL29"/>
<connect gate="B" pin="DDR0A9" pad="AK29"/>
<connect gate="B" pin="DDR0BA0" pad="AK26"/>
<connect gate="B" pin="DDR0BA1" pad="AF23"/>
<connect gate="B" pin="DDR0BA2" pad="AH25"/>
<connect gate="B" pin="DDR0CASN" pad="AK25"/>
<connect gate="B" pin="DDR0CKE" pad="AD20"/>
<connect gate="B" pin="DDR0CLK" pad="AL27"/>
<connect gate="B" pin="DDR0CLKN" pad="AK27"/>
<connect gate="B" pin="DDR0CS0N" pad="AB21"/>
<connect gate="B" pin="DDR0D0" pad="AL9"/>
<connect gate="B" pin="DDR0D1" pad="AK9"/>
<connect gate="B" pin="DDR0D10" pad="AD12"/>
<connect gate="B" pin="DDR0D11" pad="AB12"/>
<connect gate="B" pin="DDR0D12" pad="AK13"/>
<connect gate="B" pin="DDR0D13" pad="AC13"/>
<connect gate="B" pin="DDR0D14" pad="AL14"/>
<connect gate="B" pin="DDR0D15" pad="AK14"/>
<connect gate="B" pin="DDR0D16" pad="AH15"/>
<connect gate="B" pin="DDR0D17" pad="AF15"/>
<connect gate="B" pin="DDR0D18" pad="AD15"/>
<connect gate="B" pin="DDR0D19" pad="AK16"/>
<connect gate="B" pin="DDR0D2" pad="AK10"/>
<connect gate="B" pin="DDR0D20" pad="AJ16"/>
<connect gate="B" pin="DDR0D21" pad="AG16"/>
<connect gate="B" pin="DDR0D22" pad="AD16"/>
<connect gate="B" pin="DDR0D23" pad="AC16"/>
<connect gate="B" pin="DDR0D24" pad="AK19"/>
<connect gate="B" pin="DDR0D25" pad="AJ19"/>
<connect gate="B" pin="DDR0D26" pad="AH19"/>
<connect gate="B" pin="DDR0D27" pad="AF19"/>
<connect gate="B" pin="DDR0D28" pad="AD19"/>
<connect gate="B" pin="DDR0D29" pad="AC19"/>
<connect gate="B" pin="DDR0D3" pad="AJ11"/>
<connect gate="B" pin="DDR0D30" pad="AJ20"/>
<connect gate="B" pin="DDR0D31" pad="AG20"/>
<connect gate="B" pin="DDR0D4" pad="AH11"/>
<connect gate="B" pin="DDR0D5" pad="AD9"/>
<connect gate="B" pin="DDR0D6" pad="AF11"/>
<connect gate="B" pin="DDR0D7" pad="AL12"/>
<connect gate="B" pin="DDR0D8" pad="AJ12"/>
<connect gate="B" pin="DDR0D9" pad="AG12"/>
<connect gate="B" pin="DDR0DQM0" pad="AL8"/>
<connect gate="B" pin="DDR0DQM1" pad="AK12"/>
<connect gate="B" pin="DDR0DQM2" pad="AJ15"/>
<connect gate="B" pin="DDR0DQM3" pad="AK18"/>
<connect gate="B" pin="DDR0DQS0" pad="AL11"/>
<connect gate="B" pin="DDR0DQS0N" pad="AK11"/>
<connect gate="B" pin="DDR0DQS1" pad="AL15"/>
<connect gate="B" pin="DDR0DQS1N" pad="AK15"/>
<connect gate="B" pin="DDR0DQS2" pad="AL17"/>
<connect gate="B" pin="DDR0DQS2N" pad="AK17"/>
<connect gate="B" pin="DDR0DQS3" pad="AL20"/>
<connect gate="B" pin="DDR0DQS3N" pad="AK20"/>
<connect gate="B" pin="DDR0ODT0" pad="AL21"/>
<connect gate="B" pin="DDR0RASN" pad="AJ25"/>
<connect gate="B" pin="DDR0RST" pad="AA20"/>
<connect gate="B" pin="DDR0WEN" pad="AL26"/>
<connect gate="B" pin="VREFSSTLDDR0" pad="AL18"/>
<connect gate="C" pin="EMAC0GMTCLK_EMAC1RGRXC" pad="AL6"/>
<connect gate="C" pin="EMAC0MCOL_EMAC0RGRXCTL" pad="AH1"/>
<connect gate="C" pin="EMAC0MCRS_EMAC0RGRXD2" pad="AH2"/>
<connect gate="C" pin="EMAC0MRCLK_EMAC0RGTXC" pad="AK1"/>
<connect gate="C" pin="EMAC0MRXD0_EMAC0RGTXD0" pad="AK2"/>
<connect gate="C" pin="EMAC0MRXD1_EMAC0RGRXD0" pad="AL2"/>
<connect gate="C" pin="EMAC0MRXD2_EMAC0RGRXD1" pad="AL3"/>
<connect gate="C" pin="EMAC0MRXD3_EMAC1RGRXCTL" pad="AK3"/>
<connect gate="C" pin="EMAC0MRXD4_EMAC0RGRXD3" pad="AK4"/>
<connect gate="C" pin="EMAC0MRXD5_EMAC0RGTXD3" pad="AJ4"/>
<connect gate="C" pin="EMAC0MRXD6_EMAC0RGTXD2" pad="AL5"/>
<connect gate="C" pin="EMAC0MRXD7_EMAC0RGTXD1" pad="AK5"/>
<connect gate="C" pin="EMAC0MRXDV_EMAC1RGRXD1" pad="AJ6"/>
<connect gate="C" pin="EMAC0MRXER_EMAC0RGTXCTL" pad="AJ2"/>
<connect gate="C" pin="EMAC0MTCLK_EMAC0RGRXC" pad="AG4"/>
<connect gate="C" pin="EMAC0MTXD0_EMAC1RGRXD3" pad="AK6"/>
<connect gate="C" pin="EMAC0MTXD1_EMAC1RGTXD1" pad="AJ7"/>
<connect gate="C" pin="EMAC0MTXD2_EMAC1RGTXCTL" pad="AK7"/>
<connect gate="C" pin="EMAC0MTXD3_EMAC1RGTXD0" pad="AE4"/>
<connect gate="C" pin="EMAC0MTXD4_EMAC1RGTXD2" pad="AK8"/>
<connect gate="C" pin="EMAC0MTXD5_EMAC1RGTXC" pad="AJ8"/>
<connect gate="C" pin="EMAC0MTXD6_EMAC1RGRXD0" pad="AH8"/>
<connect gate="C" pin="EMAC0MTXD7_EMAC1RGTXD3" pad="AG8"/>
<connect gate="C" pin="EMAC0MTXEN_EMAC1RGRXD2" pad="AF8"/>
<connect gate="C" pin="EMACRMREFCLK" pad="AG1"/>
<connect gate="D" pin="GPMCA16" pad="M1"/>
<connect gate="D" pin="GPMCA17" pad="M2"/>
<connect gate="D" pin="GPMCA18" pad="M3"/>
<connect gate="D" pin="GPMCA19" pad="M5"/>
<connect gate="D" pin="GPMCA20" pad="N9"/>
<connect gate="D" pin="GPMCA21" pad="N1"/>
<connect gate="D" pin="GPMCA22" pad="N2"/>
<connect gate="D" pin="GPMCA23" pad="R8"/>
<connect gate="D" pin="GPMCADVNALE" pad="AA10"/>
<connect gate="D" pin="GPMCBE0NCLE" pad="Y3"/>
<connect gate="D" pin="GPMCBE1N" pad="Y11"/>
<connect gate="D" pin="GPMCCLK" pad="AB9"/>
<connect gate="D" pin="GPMCCS0N" pad="AC9"/>
<connect gate="D" pin="GPMCCS1N" pad="AA12"/>
<connect gate="D" pin="GPMCCS2N" pad="AC3"/>
<connect gate="D" pin="GPMCCS3N" pad="AF2"/>
<connect gate="D" pin="GPMCCS4N" pad="AG6"/>
<connect gate="D" pin="GPMCD0" pad="W6"/>
<connect gate="D" pin="GPMCD1" pad="W4"/>
<connect gate="D" pin="GPMCD10" pad="R6"/>
<connect gate="D" pin="GPMCD11" pad="R4"/>
<connect gate="D" pin="GPMCD12" pad="R3"/>
<connect gate="D" pin="GPMCD13" pad="R2"/>
<connect gate="D" pin="GPMCD14" pad="R1"/>
<connect gate="D" pin="GPMCD15" pad="P2"/>
<connect gate="D" pin="GPMCD2" pad="W3"/>
<connect gate="D" pin="GPMCD3" pad="U2"/>
<connect gate="D" pin="GPMCD4" pad="W9"/>
<connect gate="D" pin="GPMCD5" pad="T5"/>
<connect gate="D" pin="GPMCD6" pad="T3"/>
<connect gate="D" pin="GPMCD7" pad="T2"/>
<connect gate="D" pin="GPMCD8" pad="T1"/>
<connect gate="D" pin="GPMCD9" pad="T8"/>
<connect gate="D" pin="GPMCOEREN" pad="Y8"/>
<connect gate="D" pin="GPMCWAIT0" pad="W8"/>
<connect gate="D" pin="GPMCWEN" pad="Y5"/>
<connect gate="E" pin="MCA0ACLKR" pad="AD30"/>
<connect gate="E" pin="MCA0ACLKX" pad="AD28"/>
<connect gate="E" pin="MCA0AFSR" pad="AF30"/>
<connect gate="E" pin="MCA0AFSX" pad="AE29"/>
<connect gate="E" pin="MCA0AXR0" pad="AF29"/>
<connect gate="E" pin="MCA0AXR1" pad="AE31"/>
<connect gate="E" pin="MCA0AXR2" pad="AE30"/>
<connect gate="E" pin="MCA0AXR3" pad="AC31"/>
<connect gate="E" pin="MCA0AXR4" pad="AD26"/>
<connect gate="E" pin="MCA0AXR5" pad="AD27"/>
<connect gate="E" pin="MCA1ACLKR" pad="AD29"/>
<connect gate="E" pin="MCA1ACLKX" pad="AC23"/>
<connect gate="E" pin="MCA1AFSR" pad="AC24"/>
<connect gate="E" pin="MCA1AFSX" pad="AB22"/>
<connect gate="E" pin="MCA1AXR0" pad="Y22"/>
<connect gate="E" pin="MCA1AXR1" pad="Y21"/>
<connect gate="F" pin="SD0CLK" pad="AB30"/>
<connect gate="F" pin="SD0CMD" pad="AA29"/>
<connect gate="F" pin="SD0DAT0" pad="AA28"/>
<connect gate="F" pin="SD0DAT1SDIRQN" pad="AA26"/>
<connect gate="F" pin="SD0DAT2SDRWN" pad="Y31"/>
<connect gate="F" pin="SD0DAT3" pad="Y30"/>
<connect gate="F" pin="SD0DAT6" pad="AB31"/>
<connect gate="F" pin="SD0DAT7" pad="AC30"/>
<connect gate="F" pin="SD1CLK" pad="W30"/>
<connect gate="F" pin="SD1CMD" pad="Y29"/>
<connect gate="F" pin="SD1DAT0" pad="W31"/>
<connect gate="F" pin="SD1DAT1SDIRQN" pad="AA30"/>
<connect gate="F" pin="SD1DAT2SDRWN" pad="U29"/>
<connect gate="F" pin="SD1DAT3" pad="Y27"/>
<connect gate="F" pin="SD2DAT0" pad="AC4"/>
<connect gate="F" pin="SD2DAT1SDIRQN" pad="AC5"/>
<connect gate="F" pin="SD2DAT2SDRWN" pad="AC8"/>
<connect gate="F" pin="SD2DAT3" pad="AD1"/>
<connect gate="F" pin="SD2DAT4" pad="AD2"/>
<connect gate="F" pin="SD2DAT5" pad="AE1"/>
<connect gate="F" pin="SD2DAT6" pad="AE2"/>
<connect gate="F" pin="SD2DAT7" pad="AE3"/>
<connect gate="F" pin="SD2SCLK" pad="AC6"/>
<connect gate="G" pin="SPI0D0" pad="J28"/>
<connect gate="G" pin="SPI0D1" pad="J27"/>
<connect gate="G" pin="SPI0SCLK" pad="N24"/>
<connect gate="G" pin="SPI0SCS0N" pad="G29"/>
<connect gate="G" pin="SPI0SCS1N" pad="G28"/>
<connect gate="G" pin="SPI1D0" pad="N23"/>
<connect gate="G" pin="SPI1D1" pad="M27"/>
<connect gate="G" pin="SPI1SCLK" pad="M29"/>
<connect gate="G" pin="SPI1SCS0N" pad="J29"/>
<connect gate="H" pin="UART0CTSN" pad="D30"/>
<connect gate="H" pin="UART0DCDN" pad="E31"/>
<connect gate="H" pin="UART0DSRN" pad="E29"/>
<connect gate="H" pin="UART0DTRN" pad="E30"/>
<connect gate="H" pin="UART0RIN" pad="N26"/>
<connect gate="H" pin="UART0RTSN" pad="D31"/>
<connect gate="H" pin="UART0RXD" pad="J26"/>
<connect gate="H" pin="UART0TXD" pad="E28"/>
<connect gate="H" pin="UART2RXD" pad="L22"/>
<connect gate="H" pin="UART2TXD" pad="M21"/>
<connect gate="H" pin="USB0DRVVBUS" pad="K23"/>
<connect gate="I" pin="I2C0SCL" pad="T27"/>
<connect gate="I" pin="I2C0SDA" pad="T24"/>
<connect gate="I" pin="I2C1SCL" pad="D2"/>
<connect gate="I" pin="I2C1SDA" pad="D1"/>
<connect gate="J" pin="LDOCAPARM" pad="J19"/>
<connect gate="J" pin="LDOCAPARMRAM" pad="K20"/>
<connect gate="J" pin="LDOCAPHDVICP" pad="W23"/>
<connect gate="J" pin="LDOCAPHDVICPRAM" pad="Y24"/>
<connect gate="J" pin="LDOCAPRAM0" pad="U9"/>
<connect gate="J" pin="LDOCAPRAM1" pad="T22"/>
<connect gate="J" pin="LDOCAPRAM2" pad="AB10"/>
<connect gate="J" pin="LDOCAPSERDESCLK" pad="M24"/>
<connect gate="K" pin="VIN0ACLK" pad="C9"/>
<connect gate="K" pin="VIN0AD0" pad="B18"/>
<connect gate="K" pin="VIN0AD1" pad="A17"/>
<connect gate="K" pin="VIN0AD10BD2" pad="E16"/>
<connect gate="K" pin="VIN0AD11BD3" pad="H17"/>
<connect gate="K" pin="VIN0AD12BD4" pad="J16"/>
<connect gate="K" pin="VIN0AD13BD5" pad="H16"/>
<connect gate="K" pin="VIN0AD14BD6" pad="F13"/>
<connect gate="K" pin="VIN0AD15BD7" pad="H13"/>
<connect gate="K" pin="VIN0AD16" pad="K11"/>
<connect gate="K" pin="VIN0AD17" pad="E12"/>
<connect gate="K" pin="VIN0AD18" pad="K10"/>
<connect gate="K" pin="VIN0AD19" pad="D7"/>
<connect gate="K" pin="VIN0AD2" pad="B17"/>
<connect gate="K" pin="VIN0AD20" pad="F9"/>
<connect gate="K" pin="VIN0AD21" pad="C7"/>
<connect gate="K" pin="VIN0AD22" pad="A6"/>
<connect gate="K" pin="VIN0AD23" pad="A5"/>
<connect gate="K" pin="VIN0AD3" pad="C17"/>
<connect gate="K" pin="VIN0AD4" pad="D17"/>
<connect gate="K" pin="VIN0AD5" pad="F17"/>
<connect gate="K" pin="VIN0AD6" pad="L20"/>
<connect gate="K" pin="VIN0AD7" pad="H20"/>
<connect gate="K" pin="VIN0AD8BD0" pad="B16"/>
<connect gate="K" pin="VIN0AD9BD1" pad="C16"/>
<connect gate="K" pin="VIN0ADE" pad="C12"/>
<connect gate="K" pin="VIN0ADE1" pad="B5"/>
<connect gate="K" pin="VIN0AFLD" pad="J13"/>
<connect gate="K" pin="VIN0AFLD1" pad="B4"/>
<connect gate="K" pin="VIN0AHSYNC" pad="D13"/>
<connect gate="K" pin="VIN0AVSYNC" pad="C13"/>
<connect gate="K" pin="VIN0BCLK" pad="H12"/>
<connect gate="K" pin="VIN0BDE" pad="C5"/>
<connect gate="K" pin="VIN0BFLD" pad="A3"/>
<connect gate="L" pin="VOUT0AVID" pad="C20"/>
<connect gate="L" pin="VOUT0BCBC2" pad="F24"/>
<connect gate="L" pin="VOUT0BCBC3" pad="D21"/>
<connect gate="L" pin="VOUT0BCBC4" pad="J23"/>
<connect gate="L" pin="VOUT0BCBC5" pad="H23"/>
<connect gate="L" pin="VOUT0BCBC6" pad="J24"/>
<connect gate="L" pin="VOUT0BCBC7" pad="E24"/>
<connect gate="L" pin="VOUT0BCBC8" pad="D24"/>
<connect gate="L" pin="VOUT0BCBC9" pad="C24"/>
<connect gate="L" pin="VOUT0CLK" pad="K22"/>
<connect gate="L" pin="VOUT0FLD" pad="B3"/>
<connect gate="L" pin="VOUT0GYYC2" pad="C25"/>
<connect gate="L" pin="VOUT0GYYC3" pad="C26"/>
<connect gate="L" pin="VOUT0GYYC4" pad="E26"/>
<connect gate="L" pin="VOUT0GYYC5" pad="B26"/>
<connect gate="L" pin="VOUT0GYYC6" pad="A26"/>
<connect gate="L" pin="VOUT0GYYC7" pad="B25"/>
<connect gate="L" pin="VOUT0GYYC8" pad="B27"/>
<connect gate="L" pin="VOUT0GYYC9" pad="A27"/>
<connect gate="L" pin="VOUT0HSYNC" pad="F21"/>
<connect gate="L" pin="VOUT0RCR2" pad="C28"/>
<connect gate="L" pin="VOUT0RCR3" pad="B28"/>
<connect gate="L" pin="VOUT0RCR4" pad="B29"/>
<connect gate="L" pin="VOUT0RCR5" pad="A29"/>
<connect gate="L" pin="VOUT0RCR6" pad="C30"/>
<connect gate="L" pin="VOUT0RCR7" pad="B30"/>
<connect gate="L" pin="VOUT0RCR8" pad="A30"/>
<connect gate="L" pin="VOUT0RCR9" pad="B31"/>
<connect gate="L" pin="VOUT0VSYNC" pad="E20"/>
<connect gate="L" pin="VOUT1AVID" pad="F1"/>
<connect gate="L" pin="VOUT1BCBC0" pad="H9"/>
<connect gate="L" pin="VOUT1BCBC1" pad="D5"/>
<connect gate="L" pin="VOUT1BCBC2" pad="M8"/>
<connect gate="L" pin="VOUT1BCBC3" pad="F2"/>
<connect gate="L" pin="VOUT1BCBC4" pad="F3"/>
<connect gate="L" pin="VOUT1BCBC5" pad="G1"/>
<connect gate="L" pin="VOUT1BCBC6" pad="G2"/>
<connect gate="L" pin="VOUT1BCBC7" pad="H3"/>
<connect gate="L" pin="VOUT1BCBC8" pad="G3"/>
<connect gate="L" pin="VOUT1BCBC9" pad="H5"/>
<connect gate="L" pin="VOUT1CLK" pad="D3"/>
<connect gate="L" pin="VOUT1FLD" pad="J10"/>
<connect gate="L" pin="VOUT1GYYC0" pad="B2"/>
<connect gate="L" pin="VOUT1GYYC1" pad="A2"/>
<connect gate="L" pin="VOUT1GYYC2" pad="L2"/>
<connect gate="L" pin="VOUT1GYYC3" pad="H6"/>
<connect gate="L" pin="VOUT1GYYC4" pad="J8"/>
<connect gate="L" pin="VOUT1GYYC5" pad="J1"/>
<connect gate="L" pin="VOUT1GYYC6" pad="H4"/>
<connect gate="L" pin="VOUT1GYYC7" pad="J9"/>
<connect gate="L" pin="VOUT1GYYC8" pad="L3"/>
<connect gate="L" pin="VOUT1GYYC9" pad="K1"/>
<connect gate="L" pin="VOUT1HSYNC" pad="E2"/>
<connect gate="L" pin="VOUT1RCR0" pad="C2"/>
<connect gate="L" pin="VOUT1RCR1" pad="C1"/>
<connect gate="L" pin="VOUT1RCR2" pad="L6"/>
<connect gate="L" pin="VOUT1RCR3" pad="L4"/>
<connect gate="L" pin="VOUT1RCR4" pad="H2"/>
<connect gate="L" pin="VOUT1RCR5" pad="M11"/>
<connect gate="L" pin="VOUT1RCR6" pad="L12"/>
<connect gate="L" pin="VOUT1RCR7" pad="M10"/>
<connect gate="L" pin="VOUT1RCR8" pad="J2"/>
<connect gate="L" pin="VOUT1RCR9" pad="K2"/>
<connect gate="L" pin="VOUT1VSYNC" pad="F5"/>
<connect gate="M" pin="CVDD@1" pad="U11"/>
<connect gate="M" pin="CVDD@10" pad="P15"/>
<connect gate="M" pin="CVDD@11" pad="R15"/>
<connect gate="M" pin="CVDD@12" pad="U15"/>
<connect gate="M" pin="CVDD@13" pad="V15"/>
<connect gate="M" pin="CVDD@14" pad="P17"/>
<connect gate="M" pin="CVDD@15" pad="R17"/>
<connect gate="M" pin="CVDD@16" pad="T17"/>
<connect gate="M" pin="CVDD@17" pad="U17"/>
<connect gate="M" pin="CVDD@18" pad="V17"/>
<connect gate="M" pin="CVDD@19" pad="T18"/>
<connect gate="M" pin="CVDD@2" pad="V11"/>
<connect gate="M" pin="CVDD@20" pad="W19"/>
<connect gate="M" pin="CVDD@21" pad="Y19"/>
<connect gate="M" pin="CVDD@22" pad="W20"/>
<connect gate="M" pin="CVDD@23" pad="Y20"/>
<connect gate="M" pin="CVDD@3" pad="U12"/>
<connect gate="M" pin="CVDD@4" pad="V12"/>
<connect gate="M" pin="CVDD@5" pad="T13"/>
<connect gate="M" pin="CVDD@6" pad="W13"/>
<connect gate="M" pin="CVDD@7" pad="Y13"/>
<connect gate="M" pin="CVDD@8" pad="W14"/>
<connect gate="M" pin="CVDD@9" pad="Y14"/>
<connect gate="M" pin="CVDDARM@1" pad="M13"/>
<connect gate="M" pin="CVDDARM@2" pad="M14"/>
<connect gate="M" pin="CVDDARM@3" pad="K17"/>
<connect gate="M" pin="CVDDARM@4" pad="L17"/>
<connect gate="M" pin="CVDDARM@5" pad="M17"/>
<connect gate="M" pin="CVDDARM@6" pad="L18"/>
<connect gate="M" pin="CVDDHDVICP@1" pad="U20"/>
<connect gate="M" pin="CVDDHDVICP@2" pad="V20"/>
<connect gate="M" pin="CVDDHDVICP@3" pad="U21"/>
<connect gate="M" pin="CVDDHDVICP@4" pad="V21"/>
<connect gate="M" pin="CVDDHDVICP@5" pad="W22"/>
<connect gate="N" pin="DVDD@1" pad="M4"/>
<connect gate="N" pin="DVDD@10" pad="T26"/>
<connect gate="N" pin="DVDD@11" pad="U27"/>
<connect gate="N" pin="DVDD@12" pad="T28"/>
<connect gate="N" pin="DVDD@2" pad="L5"/>
<connect gate="N" pin="DVDD@3" pad="M6"/>
<connect gate="N" pin="DVDD@4" pad="M7"/>
<connect gate="N" pin="DVDD@5" pad="N10"/>
<connect gate="N" pin="DVDD@6" pad="N11"/>
<connect gate="N" pin="DVDD@7" pad="D16"/>
<connect gate="N" pin="DVDD@8" pad="F16"/>
<connect gate="N" pin="DVDD@9" pad="E17"/>
<connect gate="N" pin="DVDDC@1" pad="D12"/>
<connect gate="N" pin="DVDDC@2" pad="F12"/>
<connect gate="N" pin="DVDDC@3" pad="G12"/>
<connect gate="N" pin="DVDDC@4" pad="E13"/>
<connect gate="N" pin="DVDDC@5" pad="G13"/>
<connect gate="N" pin="DVDDDDR0@1" pad="AB14"/>
<connect gate="N" pin="DVDDDDR0@10" pad="AC17"/>
<connect gate="N" pin="DVDDDDR0@11" pad="AB18"/>
<connect gate="N" pin="DVDDDDR0@12" pad="AC18"/>
<connect gate="N" pin="DVDDDDR0@2" pad="AB15"/>
<connect gate="N" pin="DVDDDDR0@3" pad="AC15"/>
<connect gate="N" pin="DVDDDDR0@4" pad="AE15"/>
<connect gate="N" pin="DVDDDDR0@5" pad="AG15"/>
<connect gate="N" pin="DVDDDDR0@6" pad="AE16"/>
<connect gate="N" pin="DVDDDDR0@7" pad="AF16"/>
<connect gate="N" pin="DVDDDDR0@8" pad="AH16"/>
<connect gate="N" pin="DVDDDDR0@9" pad="AB17"/>
<connect gate="N" pin="DVDDGPMC@1" pad="T4"/>
<connect gate="N" pin="DVDDGPMC@2" pad="R5"/>
<connect gate="N" pin="DVDDGPMC@3" pad="T6"/>
<connect gate="N" pin="DVDDGPMC@4" pad="R7"/>
<connect gate="N" pin="DVDDGPMC@5" pad="T7"/>
<connect gate="N" pin="DVDDRGMII@1" pad="Y4"/>
<connect gate="N" pin="DVDDRGMII@2" pad="W5"/>
<connect gate="N" pin="DVDDRGMII@3" pad="Y6"/>
<connect gate="N" pin="DVDDRGMII@4" pad="W7"/>
<connect gate="N" pin="DVDDRGMII@5" pad="Y7"/>
<connect gate="N" pin="DVDDSD@1" pad="T25"/>
<connect gate="N" pin="DVDDSD@2" pad="U25"/>
<connect gate="O" pin="VDDA1P8@1" pad="R9"/>
<connect gate="O" pin="VDDA1P8@2" pad="T9"/>
<connect gate="O" pin="VDDA1P8@3" pad="T10"/>
<connect gate="O" pin="VDDA1P8@4" pad="N22"/>
<connect gate="O" pin="VDDA1P8@5" pad="P23"/>
<connect gate="O" pin="VDDA1P8@6" pad="M25"/>
<connect gate="O" pin="VDDA1P8@7" pad="N25"/>
<connect gate="O" pin="VDDAARMPLL1P8" pad="L19"/>
<connect gate="O" pin="VDDAAUDIOPLL1P8" pad="V9"/>
<connect gate="O" pin="VDDACSI21P8" pad="W10"/>
<connect gate="O" pin="VDDADDRPLL1P8" pad="AA19"/>
<connect gate="O" pin="VDDAHDDAC1P1" pad="K16"/>
<connect gate="O" pin="VDDAHDDAC1P8" pad="L14"/>
<connect gate="O" pin="VDDAHDDACREF1P8" pad="L15"/>
<connect gate="O" pin="VDDAHDMI1P8" pad="K14"/>
<connect gate="O" pin="VDDAHDVICPPLL1P8" pad="T23"/>
<connect gate="O" pin="VDDAL3L41P8" pad="W11"/>
<connect gate="O" pin="VDDAPCIE1P8" pad="M26"/>
<connect gate="O" pin="VDDAUSB01P8" pad="K19"/>
<connect gate="O" pin="VDDAUSB11P8" pad="J17"/>
<connect gate="O" pin="VDDAUSB3P3@1" pad="M19"/>
<connect gate="O" pin="VDDAUSB3P3@2" pad="M20"/>
<connect gate="O" pin="VDDAVDAC1P8" pad="J14"/>
<connect gate="O" pin="VDDAVIDPLL1P8" pad="L13"/>
<connect gate="O" pin="VDDSOSC01P8" pad="P21"/>
<connect gate="O" pin="VDDSOSC11P8" pad="P20"/>
<connect gate="P" pin="VSS@1" pad="A1"/>
<connect gate="P" pin="VSS@10" pad="AD6"/>
<connect gate="P" pin="VSS@100" pad="AA27"/>
<connect gate="P" pin="VSS@101" pad="AE27"/>
<connect gate="P" pin="VSS@102" pad="Y28"/>
<connect gate="P" pin="VSS@103" pad="AE28"/>
<connect gate="P" pin="VSS@104" pad="A31"/>
<connect gate="P" pin="VSS@105" pad="AL31"/>
<connect gate="P" pin="VSS@11" pad="AE6"/>
<connect gate="P" pin="VSS@12" pad="E7"/>
<connect gate="P" pin="VSS@13" pad="F7"/>
<connect gate="P" pin="VSS@14" pad="G7"/>
<connect gate="P" pin="VSS@15" pad="H7"/>
<connect gate="P" pin="VSS@16" pad="J7"/>
<connect gate="P" pin="VSS@17" pad="AD7"/>
<connect gate="P" pin="VSS@18" pad="AE7"/>
<connect gate="P" pin="VSS@19" pad="AF7"/>
<connect gate="P" pin="VSS@2" pad="AL1"/>
<connect gate="P" pin="VSS@20" pad="AG7"/>
<connect gate="P" pin="VSS@21" pad="AH7"/>
<connect gate="P" pin="VSS@22" pad="D8"/>
<connect gate="P" pin="VSS@23" pad="E8"/>
<connect gate="P" pin="VSS@24" pad="F8"/>
<connect gate="P" pin="VSS@25" pad="G8"/>
<connect gate="P" pin="VSS@26" pad="AE8"/>
<connect gate="P" pin="VSS@27" pad="AE9"/>
<connect gate="P" pin="VSS@28" pad="P11"/>
<connect gate="P" pin="VSS@29" pad="R11"/>
<connect gate="P" pin="VSS@3" pad="AD3"/>
<connect gate="P" pin="VSS@30" pad="T11"/>
<connect gate="P" pin="VSS@31" pad="AG11"/>
<connect gate="P" pin="VSS@32" pad="P12"/>
<connect gate="P" pin="VSS@33" pad="R12"/>
<connect gate="P" pin="VSS@34" pad="T12"/>
<connect gate="P" pin="VSS@35" pad="AE12"/>
<connect gate="P" pin="VSS@36" pad="AF12"/>
<connect gate="P" pin="VSS@37" pad="AH12"/>
<connect gate="P" pin="VSS@38" pad="N13"/>
<connect gate="P" pin="VSS@39" pad="AA13"/>
<connect gate="P" pin="VSS@4" pad="G4"/>
<connect gate="P" pin="VSS@40" pad="N14"/>
<connect gate="P" pin="VSS@41" pad="P14"/>
<connect gate="P" pin="VSS@42" pad="R14"/>
<connect gate="P" pin="VSS@43" pad="T14"/>
<connect gate="P" pin="VSS@44" pad="U14"/>
<connect gate="P" pin="VSS@45" pad="AA14"/>
<connect gate="P" pin="VSS@46" pad="T15"/>
<connect gate="P" pin="VSS@47" pad="AA15"/>
<connect gate="P" pin="VSS@48" pad="L16"/>
<connect gate="P" pin="VSS@49" pad="M16"/>
<connect gate="P" pin="VSS@5" pad="AD4"/>
<connect gate="P" pin="VSS@50" pad="N16"/>
<connect gate="P" pin="VSS@51" pad="T16"/>
<connect gate="P" pin="VSS@52" pad="W16"/>
<connect gate="P" pin="VSS@53" pad="Y16"/>
<connect gate="P" pin="VSS@54" pad="AA16"/>
<connect gate="P" pin="VSS@55" pad="N17"/>
<connect gate="P" pin="VSS@56" pad="W17"/>
<connect gate="P" pin="VSS@57" pad="Y17"/>
<connect gate="P" pin="VSS@58" pad="AA17"/>
<connect gate="P" pin="VSS@59" pad="P18"/>
<connect gate="P" pin="VSS@6" pad="G5"/>
<connect gate="P" pin="VSS@60" pad="R18"/>
<connect gate="P" pin="VSS@61" pad="U18"/>
<connect gate="P" pin="VSS@62" pad="V18"/>
<connect gate="P" pin="VSS@63" pad="AA18"/>
<connect gate="P" pin="VSS@64" pad="T19"/>
<connect gate="P" pin="VSS@65" pad="AE19"/>
<connect gate="P" pin="VSS@66" pad="AG19"/>
<connect gate="P" pin="VSS@67" pad="F20"/>
<connect gate="P" pin="VSS@68" pad="G20"/>
<connect gate="P" pin="VSS@69" pad="R20"/>
<connect gate="P" pin="VSS@7" pad="AD5"/>
<connect gate="P" pin="VSS@70" pad="T20"/>
<connect gate="P" pin="VSS@71" pad="AE20"/>
<connect gate="P" pin="VSS@72" pad="AF20"/>
<connect gate="P" pin="VSS@73" pad="AH20"/>
<connect gate="P" pin="VSS@74" pad="E21"/>
<connect gate="P" pin="VSS@75" pad="R21"/>
<connect gate="P" pin="VSS@76" pad="T21"/>
<connect gate="P" pin="VSS@77" pad="G23"/>
<connect gate="P" pin="VSS@78" pad="U23"/>
<connect gate="P" pin="VSS@79" pad="AE23"/>
<connect gate="P" pin="VSS@8" pad="AE5"/>
<connect gate="P" pin="VSS@80" pad="G24"/>
<connect gate="P" pin="VSS@81" pad="AD24"/>
<connect gate="P" pin="VSS@82" pad="AE24"/>
<connect gate="P" pin="VSS@83" pad="AF24"/>
<connect gate="P" pin="VSS@84" pad="AG24"/>
<connect gate="P" pin="VSS@85" pad="D25"/>
<connect gate="P" pin="VSS@86" pad="E25"/>
<connect gate="P" pin="VSS@87" pad="F25"/>
<connect gate="P" pin="VSS@88" pad="G25"/>
<connect gate="P" pin="VSS@89" pad="Y25"/>
<connect gate="P" pin="VSS@9" pad="G6"/>
<connect gate="P" pin="VSS@90" pad="AC25"/>
<connect gate="P" pin="VSS@91" pad="AD25"/>
<connect gate="P" pin="VSS@92" pad="AE25"/>
<connect gate="P" pin="VSS@93" pad="AF25"/>
<connect gate="P" pin="VSS@94" pad="AG25"/>
<connect gate="P" pin="VSS@95" pad="G26"/>
<connect gate="P" pin="VSS@96" pad="H26"/>
<connect gate="P" pin="VSS@97" pad="Y26"/>
<connect gate="P" pin="VSS@98" pad="AE26"/>
<connect gate="P" pin="VSS@99" pad="G27"/>
<connect gate="P" pin="VSSAAUXOSC" pad="U30"/>
<connect gate="P" pin="VSSACSI2@1" pad="AC7"/>
<connect gate="P" pin="VSSACSI2@2" pad="V14"/>
<connect gate="P" pin="VSSADEVOSC" pad="G30"/>
<connect gate="P" pin="VSSAHDMI@1" pad="H8"/>
<connect gate="P" pin="VSSAHDMI@2" pad="G9"/>
<connect gate="P" pin="VSSAUSB@1" pad="N19"/>
<connect gate="P" pin="VSSAUSB@2" pad="D20"/>
<connect gate="P" pin="VSSAUSB@3" pad="N20"/>
<connect gate="P" pin="VSSAVDAC" pad="C8"/>
<connect gate="Q" pin="RSV4" pad="G17"/>
<connect gate="Q" pin="RSV42" pad="AK21"/>
<connect gate="Q" pin="RSV5" pad="G16"/>
<connect gate="Q" pin="RSV54" pad="M28"/>
<connect gate="Q" pin="RSV55" pad="N27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS8684" prefix="IC">
<description>&lt;b&gt;ADS868x 16-Bit, 500-kSPS, 4-Channel, Single-Supply, SAR ADCs with Bipolar Input Ranges&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/ads8688.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ADS8684"/>
</gates>
<devices>
<device name="" package="DBT_R-PDSO-G38">
<connects>
<connect gate="G$1" pin="!CS" pad="38"/>
<connect gate="G$1" pin="!REFSEL" pad="4"/>
<connect gate="G$1" pin="!RST!/!PD" pad="2"/>
<connect gate="G$1" pin="AIN_0GND" pad="17"/>
<connect gate="G$1" pin="AIN_0P" pad="16"/>
<connect gate="G$1" pin="AIN_1GND" pad="19"/>
<connect gate="G$1" pin="AIN_1P" pad="18"/>
<connect gate="G$1" pin="AIN_2GND" pad="20"/>
<connect gate="G$1" pin="AIN_2P" pad="21"/>
<connect gate="G$1" pin="AIN_3GND" pad="22"/>
<connect gate="G$1" pin="AIN_3P" pad="23"/>
<connect gate="G$1" pin="AUX_GND" pad="11"/>
<connect gate="G$1" pin="AUX_IN" pad="10"/>
<connect gate="G$1" pin="DAISY" pad="3"/>
<connect gate="G$1" pin="DNC" pad="35"/>
<connect gate="G$1" pin="GNDA" pad="8"/>
<connect gate="G$1" pin="GNDA@1" pad="28"/>
<connect gate="G$1" pin="GNDA@2" pad="29"/>
<connect gate="G$1" pin="GNDA@3" pad="31"/>
<connect gate="G$1" pin="GNDA@4" pad="32"/>
<connect gate="G$1" pin="GNDD" pad="33"/>
<connect gate="G$1" pin="NC@1" pad="12"/>
<connect gate="G$1" pin="NC@2" pad="13"/>
<connect gate="G$1" pin="NC@3" pad="14"/>
<connect gate="G$1" pin="NC@4" pad="15"/>
<connect gate="G$1" pin="NC@5" pad="24"/>
<connect gate="G$1" pin="NC@6" pad="25"/>
<connect gate="G$1" pin="NC@7" pad="26"/>
<connect gate="G$1" pin="NC@8" pad="27"/>
<connect gate="G$1" pin="REFCAP" pad="7"/>
<connect gate="G$1" pin="REFGND" pad="6"/>
<connect gate="G$1" pin="REFIO" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="37"/>
<connect gate="G$1" pin="SDI" pad="1"/>
<connect gate="G$1" pin="SDO" pad="36"/>
<connect gate="G$1" pin="VDDA" pad="9"/>
<connect gate="G$1" pin="VDDA@1" pad="30"/>
<connect gate="G$1" pin="VDDD" pad="34"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS8688" prefix="IC">
<description>&lt;b&gt;ADS868x 16-Bit, 500-kSPS, 8-Channel, Single-Supply, SAR ADCs with Bipolar Input Ranges&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/ads8688.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ADS8688"/>
</gates>
<devices>
<device name="" package="DBT_R-PDSO-G38">
<connects>
<connect gate="G$1" pin="!CS" pad="38"/>
<connect gate="G$1" pin="!REFSEL" pad="4"/>
<connect gate="G$1" pin="!RST!/!PD" pad="2"/>
<connect gate="G$1" pin="AIN_0GND" pad="17"/>
<connect gate="G$1" pin="AIN_0P" pad="16"/>
<connect gate="G$1" pin="AIN_1GND" pad="19"/>
<connect gate="G$1" pin="AIN_1P" pad="18"/>
<connect gate="G$1" pin="AIN_2GND" pad="20"/>
<connect gate="G$1" pin="AIN_2P" pad="21"/>
<connect gate="G$1" pin="AIN_3GND" pad="22"/>
<connect gate="G$1" pin="AIN_3P" pad="23"/>
<connect gate="G$1" pin="AIN_4GND" pad="24"/>
<connect gate="G$1" pin="AIN_4P" pad="25"/>
<connect gate="G$1" pin="AIN_5GND" pad="26"/>
<connect gate="G$1" pin="AIN_5P" pad="27"/>
<connect gate="G$1" pin="AIN_6GND" pad="13"/>
<connect gate="G$1" pin="AIN_6P" pad="12"/>
<connect gate="G$1" pin="AIN_7GND" pad="15"/>
<connect gate="G$1" pin="AIN_7P" pad="14"/>
<connect gate="G$1" pin="AUX_GND" pad="11"/>
<connect gate="G$1" pin="AUX_IN" pad="10"/>
<connect gate="G$1" pin="DAISY" pad="3"/>
<connect gate="G$1" pin="DNC" pad="35"/>
<connect gate="G$1" pin="GNDA" pad="8"/>
<connect gate="G$1" pin="GNDA@1" pad="28"/>
<connect gate="G$1" pin="GNDA@2" pad="29"/>
<connect gate="G$1" pin="GNDA@3" pad="31"/>
<connect gate="G$1" pin="GNDA@4" pad="32"/>
<connect gate="G$1" pin="GNDD" pad="33"/>
<connect gate="G$1" pin="REFCAP" pad="7"/>
<connect gate="G$1" pin="REFGND" pad="6"/>
<connect gate="G$1" pin="REFIO" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="37"/>
<connect gate="G$1" pin="SDI" pad="1"/>
<connect gate="G$1" pin="SDO" pad="36"/>
<connect gate="G$1" pin="VDDA" pad="9"/>
<connect gate="G$1" pin="VDDA@1" pad="30"/>
<connect gate="G$1" pin="VDDD" pad="34"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ADS7042" prefix="IC">
<description>&lt;b&gt;ADS7042 Ultra-Low Power, Ultra-Small Size, 12-Bit, 1-MSPS, SAR ADC&lt;/b&gt;&lt;p&gt;
Soure: &lt;a href="http://www.ti.com/lit/ds/symlink/ads7042.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ADS7042"/>
</gates>
<devices>
<device name="DCU" package="DCU_(R-PDSO-G8)">
<connects>
<connect gate="G$1" pin="!SC" pad="4"/>
<connect gate="G$1" pin="AINM" pad="5"/>
<connect gate="G$1" pin="AINP" pad="6"/>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="SCLK" pad="2"/>
<connect gate="G$1" pin="SDO" pad="3"/>
<connect gate="G$1" pin="VDDA" pad="7"/>
<connect gate="G$1" pin="VDDD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="RUG" package="RUG_(R-PQFP-N8)">
<connects>
<connect gate="G$1" pin="!SC" pad="1"/>
<connect gate="G$1" pin="AINM" pad="8"/>
<connect gate="G$1" pin="AINP" pad="7"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="SCLK" pad="3"/>
<connect gate="G$1" pin="SDO" pad="2"/>
<connect gate="G$1" pin="VDDA" pad="6"/>
<connect gate="G$1" pin="VDDD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
