<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-3.81" y1="73.66" x2="-3.81" y2="0" width="0.3048" layer="20"/>
<wire x1="-3.81" y1="0" x2="54.61" y2="0" width="0.3048" layer="20"/>
<wire x1="54.61" y1="0" x2="54.61" y2="73.66" width="0.3048" layer="20"/>
<wire x1="54.61" y1="73.66" x2="-3.81" y2="73.66" width="0.3048" layer="20"/>
<text>MSP-EXP430F5529LP</text>
<text>5V</text>
<text>GND</text>
<text>P6.0</text>
<text>P6.1</text>
<text>P6.2</text>
<text>P6.3</text>
<text>P6.4</text>
<text>P7.0</text>
<text>P3.6</text>
<text>P3.5</text>
<text>P8.2</text>
<text>P3.7</text>
<text>P4.0</text>
<text>P4.3</text>
<text>P1.2</text>
<text>P1.3</text>
<text>P1.4</text>
<text>P1.5</text>
<text>P2.4</text>
<text>P2.5</text>
<text>GND</text>
<text>P2.0</text>
<text>P2.2</text>
<text>P7.4</text>
<text>RST</text>
<text>P3.0</text>
<text>P3.1</text>
<text>P2.6</text>
<text>P2.3</text>
<text>P8.1</text>
<text>P4.1</text>
<text>P4.2</text>
<text>P2.7</text>
<text>P3.2</text>
<text>P6.6</text>
<text>P1.6</text>
<text>P3.3</text>
<text>P3.4</text>
<text>P6.5</text>
<text>3V3</text>
<text>GND</text>
<text>3V3</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>GND</text>
<text>P4.7</text>
<text>P2.1</text>
<text>P1.1</text>
<text>P1.0</text>
<text>3V3</text>
<text>5V</text>
<text>TXD &gt;&gt;</text>
<text>RXD &lt;&lt;</text>
<text>RTS &gt;&gt;</text>
<text>CTS &lt;&lt;</text>
<text>SBW TST</text>
<text>SBW RST</text>
<text>BSL</text>
<text>RST</text>
<text>Rev1.5</text>
<text>LaunchPad</text>
<text>eZ-FET lite</text>
<text>USB Hub</text>
<text>GND</text>
</plain>
<libraries>
<library name="Project7264">
<packages>
<package name="TPD2E001-DRL">
<description>TPD2E001 ESD-protection diode array,DRL-Package, RM  0,5mm, H=0,6mm</description>
</package>
</packages>
</library>
<library name="MSP430_Lab">
<packages>
<package name="TILOGO_SMALL">
</package>
</packages>
</library>
<library name="sti_logo">
<packages>
<package name="LOGO16_TPLACE">
</package>
</packages>
</library>
<library name="electricalmeter">
<packages>
<package name="PBTH">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="A/3216-18R">
<description>&lt;b&gt;Chip Capacitor Type KEMET A / EIA 3216-18 reflow solder&lt;/b&gt;&lt;p&gt;KEMET S / EIA 3216-12</description>
</package>
</packages>
</library>
<library name="CAP">
<packages>
<package name="CSMD0805">
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
<library name="TI_MSP430_v16_intern">
<packages>
<package name="PN80">
<description>*** TI: PN *** JEDEC: S-PQFP-G80 *** 80 PINS ***</description>
</package>
<package name="RGC64">
<description>*** TI: RGC *** JEDEC: S-PQFP-N64 *** 64 PINS *** ---&gt; PIN 65 (exposed thermal die pad) should be connected with GND</description>
</package>
</packages>
</library>
<library name="jumper">
<packages>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP1M">
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="texas">
<packages>
<package name="RHB_S-PQFP-N32">
<description>&lt;b&gt;RHB (S-PQFP-N32)&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/tusb2046b.pdf</description>
</package>
</packages>
</library>
<library name="usb_con-update">
<packages>
<package name="HIROSE-ZX62R-B-5P">
</package>
</packages>
</library>
<library name="tps62231dry">
<packages>
<package name="DRY6">
</package>
</packages>
</library>
<library name="MSP-EXP430F5659">
<packages>
<package name="L-NR3010">
</package>
</packages>
</library>
<library name="TI-LaunchPad-Eagle">
<packages>
<package name="LOGO-ROCKET-10X7MM-BRD">
<description>&lt;b&gt;TI LaunchPad Rocket for the PCB&lt;/b&gt;

&lt;p&gt;
Based on TI's LaunchPad Rocket from &lt;a href="www.ti.com/LaunchPad"&gt;www.ti.com/LaunchPad&lt;/a&gt;
&lt;/p&gt;

&lt;p&gt;
Usage:
&lt;ol&gt;
&lt;li&gt;Place this component on Eagle Board Layout&lt;/li&gt;
&lt;li&gt;Or better: Place it on the schematic so the logo is there too!&lt;/li&gt;
&lt;li&gt;There are different sizes / footprints available&lt;/li&gt;
&lt;/ol&gt;
&lt;/p&gt;

&lt;p&gt;
As far as I know the LaunchPad rocket is released by TI under the Creative Commons license.
&lt;/p&gt;

&lt;p&gt;
Check for updates and leave me feedback: &lt;a href="https://github.com/ucdude"&gt;github.com/ucdude&lt;/a&gt;
&lt;br&gt; Happy hacking - ucDude, Nov 2012
&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="standoff">
<packages>
<package name="MOUNTHOLE_110MIL">
</package>
</packages>
</library>
<library name="microcrystal">
<packages>
<package name="MS3V-T1R">
</package>
</packages>
</library>
<library name="murata">
<packages>
<package name="MURATA-FILTER_CSTCR">
<description>Source: http://search.murata.co.jp/Ceramy/CatalogshowpageAction.do?sDirnm=A07X&amp;sFilnm=81G07006&amp;sType=2&amp;sLang=en&amp;sNHinnm=CSTCR6M00G53Z-R0&amp;sCapt=Standard_Land_Pattern_Dimensions</description>
</package>
</packages>
</library>
<library name="LP_Silkscreen">
<packages>
<package name="MS_TM">
</package>
<package name="5529_REAR_SILK_REV1_5_FINAL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$5" library="MSP430_Lab" package="TILOGO_SMALL" value=""/>
<element name="U$1" library="sti_logo" package="LOGO16_TPLACE" value=""/>
<element name="S2" library="electricalmeter" package="PBTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="electricalmeter" package="PBTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="C15" library="rcl" package="C0402" value="220n">
<attribute name="NAME"/>
</element>
<element name="C16" library="rcl" package="C0402" value="220n">
<attribute name="NAME"/>
</element>
<element name="R27" library="rcl" package="R0402" value="47k">
<attribute name="NAME"/>
</element>
<element name="C17" library="rcl" package="C0402" value="1n">
<attribute name="NAME"/>
</element>
<element name="C18" library="rcl" package="C0402" value="470n">
<attribute name="NAME"/>
</element>
<element name="C19" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="R28" library="rcl" package="R0402" value="0R">
<attribute name="NAME"/>
</element>
<element name="R29" library="rcl" package="R0402" value="470R"/>
<element name="R30" library="rcl" package="R0402" value="470R"/>
<element name="C25" library="rcl" package="C0402" value="12p"/>
<element name="C26" library="rcl" package="C0402" value="12p"/>
<element name="S3" library="electricalmeter" package="PBTH" value="RST">
<attribute name="NAME"/>
</element>
<element name="C29" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="C30" library="rcl" package="A/3216-18R" value="10u">
<attribute name="NAME"/>
</element>
<element name="U6" library="TI_MSP430_v16_intern" package="PN80" value="MSP430F5529IPNR">
<attribute name="NAME"/>
</element>
<element name="J10" library="pinhead" package="1X03" value="PWR">
<attribute name="NAME"/>
</element>
<element name="J1" library="pinhead" package="2X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="pinhead" package="2X10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="jumper" package="JP1" value="LED1_PWR">
<attribute name="NAME"/>
</element>
<element name="C101" library="rcl" package="C0402" value="470n"/>
<element name="C102" library="rcl" package="C0402" value="220n"/>
<element name="C103" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="C104" library="rcl" package="A/3216-18R" value="10u">
<attribute name="NAME"/>
</element>
<element name="C107" library="rcl" package="C0402" value="220n"/>
<element name="R101" library="rcl" package="R0402" value="470"/>
<element name="R102" library="rcl" package="R0402" value="390"/>
<element name="LED101" library="led" package="CHIP-LED0603" value="red">
<attribute name="NAME"/>
</element>
<element name="LED102" library="led" package="CHIP-LED0603" value="green">
<attribute name="NAME"/>
</element>
<element name="C112" library="rcl" package="C0402" value="1n"/>
<element name="R109" library="rcl" package="R0402" value="47k">
<attribute name="NAME"/>
</element>
<element name="R121" library="rcl" package="R0402" value="220k"/>
<element name="R122" library="rcl" package="R0402" value="220k"/>
<element name="C122" library="rcl" package="C0402" value="33p">
<attribute name="NAME"/>
</element>
<element name="R124" library="rcl" package="R0402" value="240k"/>
<element name="R125" library="rcl" package="R0402" value="150k"/>
<element name="C123" library="rcl" package="C0402" value="33p">
<attribute name="NAME"/>
</element>
<element name="C121" library="rcl" package="C0402" value="100n"/>
<element name="MSP101" library="TI_MSP430_v16_intern" package="RGC64" value="MSP430F5528IRGC">
<attribute name="NAME"/>
</element>
<element name="Q101" library="murata" package="MURATA-FILTER_CSTCR" value="PIEZO_CSTCR4M00G15L99">
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="25M8759"/>
<attribute name="MPN" value="CSTCR6M00G53-R0"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1170434"/>
</element>
<element name="C113" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="IC401" library="texas" package="RHB_S-PQFP-N32" value="TUSB2046BIRHBIRHB">
<attribute name="OC_NEWARK" value="14N8499"/>
<attribute name="MPN" value="TUSB2046BIRHBT"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1610201"/>
</element>
<element name="U402" library="tps62231dry" package="DRY6" value="TPS62237DRY">
<attribute name="DATASHEETURL" value="http://www.ti.com/lit/gpn/TPS62231"/>
<attribute name="PIN_COUNT" value="6"/>
<attribute name="GENERIC_PART_NUMBER" value="TPS62231"/>
<attribute name="DESCRIPTION" value="3 MHz Ultra Small Step Down Converter in 1x1.5 SON Package"/>
<attribute name="FAMILY_NAME" value="STEP-DOWN REGULATOR"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="INDUSTRY_STD_PKG_TYPE" value="SON"/>
<attribute name="VENDOR" value="Texas Instuments"/>
<attribute name="VALUE" value="TPS6223xDRY"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="tps62231_dry_6"/>
<attribute name="PACKAGE_DESIGNATOR" value="DRY"/>
<attribute name="NAME"/>
</element>
<element name="J401" library="usb_con-update" package="HIROSE-ZX62R-B-5P" value="">
<attribute name="NAME"/>
</element>
<element name="C404" library="CAP" package="CSMD0805" value="1u">
<attribute name="NAME"/>
</element>
<element name="C401" library="CAP" package="CSMD0805" value="1u"/>
<element name="Q401" library="murata" package="MURATA-FILTER_CSTCR" value="CSTCR6M00G15L99">
<attribute name="OC_NEWARK" value="25M8759"/>
<attribute name="MPN" value="CSTCR6M00G53-R0"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1170434"/>
<attribute name="NAME"/>
</element>
<element name="U404" library="Project7264" package="TPD2E001-DRL" value="TPD2E001DRLR">
<attribute name="NAME"/>
</element>
<element name="R14" library="rcl" package="R0402" value="100R">
<attribute name="NAME"/>
</element>
<element name="S5" library="electricalmeter" package="PBTH" value="BSL">
<attribute name="NAME"/>
</element>
<element name="R15" library="rcl" package="R0402" value="1k4">
<attribute name="NAME"/>
</element>
<element name="R16" library="rcl" package="R0402" value="1M">
<attribute name="NAME"/>
</element>
<element name="Q4" library="murata" package="MURATA-FILTER_CSTCR" value="CSTCR4M00G15L99">
<attribute name="OC_NEWARK" value="25M8759"/>
<attribute name="MPN" value="CSTCR6M00G53-R0"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1170434"/>
<attribute name="NAME"/>
</element>
<element name="JP1" library="jumper" package="JP1M" value="+5V"/>
<element name="JP2" library="jumper" package="JP1M" value="+3V3"/>
<element name="L401" library="MSP-EXP430F5659" package="L-NR3010" value="2.2uH (NR3010T2R2M)">
<attribute name="NAME"/>
</element>
<element name="R105" library="rcl" package="R0402" value="1k4"/>
<element name="R106" library="rcl" package="R0402" value="1M">
<attribute name="NAME"/>
</element>
<element name="C402" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="C405" library="rcl" package="C0402" value="22p">
<attribute name="NAME"/>
</element>
<element name="C406" library="rcl" package="C0402" value="22p"/>
<element name="R405" library="rcl" package="R0402" value="22R"/>
<element name="R406" library="rcl" package="R0402" value="22R"/>
<element name="R403" library="rcl" package="R0402" value="1k5"/>
<element name="R410" library="rcl" package="R0402" value="22R"/>
<element name="R411" library="rcl" package="R0402" value="22R"/>
<element name="R416" library="rcl" package="R0402" value="22R"/>
<element name="R417" library="rcl" package="R0402" value="22R"/>
<element name="R414" library="rcl" package="R0402" value="15k"/>
<element name="R415" library="rcl" package="R0402" value="15k">
<attribute name="NAME"/>
</element>
<element name="R418" library="rcl" package="R0402" value="15k">
<attribute name="NAME"/>
</element>
<element name="R419" library="rcl" package="R0402" value="15k">
<attribute name="NAME"/>
</element>
<element name="C409" library="rcl" package="C0402" value="22p">
<attribute name="NAME"/>
</element>
<element name="C410" library="rcl" package="C0402" value="22p">
<attribute name="NAME"/>
</element>
<element name="C411" library="rcl" package="C0402" value="22p"/>
<element name="C412" library="rcl" package="C0402" value="22p">
<attribute name="NAME"/>
</element>
<element name="R402" library="rcl" package="R0402" value="10k">
<attribute name="NAME"/>
</element>
<element name="R401" library="rcl" package="R0402" value="33R"/>
<element name="C403" library="rcl" package="A/3216-18R" value="4u7">
<attribute name="NAME"/>
</element>
<element name="R407" library="rcl" package="R0402" value="1k5">
<attribute name="NAME"/>
</element>
<element name="TP105" library="pinhead" package="1X01" value="TEST_PIN2"/>
<element name="TP110" library="pinhead" package="1X01" value="TEST_PIN2">
<attribute name="NAME"/>
</element>
<element name="TP106" library="pinhead" package="1X01" value="TEST_PIN2"/>
<element name="TP107" library="pinhead" package="1X01" value="TEST_PIN2"/>
<element name="TP108" library="pinhead" package="1X01" value="TEST_PIN2"/>
<element name="TP109" library="pinhead" package="1X01" value="TEST_PIN2"/>
<element name="TP104" library="pinhead" package="1X01" value="TEST_PIN2">
<attribute name="NAME"/>
</element>
<element name="R404" library="rcl" package="R0402" value="47k">
<attribute name="NAME"/>
</element>
<element name="C408" library="rcl" package="C0402" value="100n"/>
<element name="C407" library="rcl" package="C0402" value="100n"/>
<element name="R409" library="rcl" package="R0402" value="15k"/>
<element name="R408" library="rcl" package="R0402" value="15k"/>
<element name="R413" library="rcl" package="R0402" value="15k"/>
<element name="R412" library="rcl" package="R0402" value="15k"/>
<element name="R104" library="rcl" package="R0402" value="27R"/>
<element name="C111" library="rcl" package="C0402" value="10p"/>
<element name="R103" library="rcl" package="R0402" value="27R">
<attribute name="NAME"/>
</element>
<element name="C110" library="rcl" package="C0402" value="10p"/>
<element name="R31" library="rcl" package="R0402" value="27R">
<attribute name="NAME"/>
</element>
<element name="R32" library="rcl" package="R0402" value="27R">
<attribute name="NAME"/>
</element>
<element name="C23" library="rcl" package="C0402" value="10p"/>
<element name="C24" library="rcl" package="C0402" value="10p"/>
<element name="C27" library="rcl" package="A/3216-18R" value="4u7">
<attribute name="NAME"/>
</element>
<element name="J3" library="pinhead" package="1X03" value="PWR">
<attribute name="NAME"/>
</element>
<element name="C20" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="C21" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="C28" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="C31" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
</element>
<element name="JP6.4" library="jumper" package="JP1M" value="RTS"/>
<element name="JP6.3" library="jumper" package="JP1M" value="CTS"/>
<element name="U$2" library="MSP430_Lab" package="TILOGO_SMALL" value=""/>
<element name="DRAW2" library="TI-LaunchPad-Eagle" package="LOGO-ROCKET-10X7MM-BRD" value=""/>
<element name="DRAW1" library="TI-LaunchPad-Eagle" package="LOGO-ROCKET-10X7MM-BRD" value=""/>
<element name="Q2" library="microcrystal" package="MS3V-T1R" value="32.768kHz">
<attribute name="NAME"/>
</element>
<element name="STAND1" library="standoff" package="MOUNTHOLE_110MIL" value=""/>
<element name="STAND2" library="standoff" package="MOUNTHOLE_110MIL" value=""/>
<element name="STAND3" library="standoff" package="MOUNTHOLE_110MIL" value=""/>
<element name="STAND4" library="standoff" package="MOUNTHOLE_110MIL" value=""/>
<element name="JP4.1" library="jumper" package="JP1M" value="SBW_TST"/>
<element name="JP4.2" library="jumper" package="JP1M" value="SBW_RST"/>
<element name="JP6.1" library="jumper" package="JP1M" value="TXD"/>
<element name="JP6.2" library="jumper" package="JP1M" value="RXD"/>
<element name="JP4.3" library="jumper" package="JP1M" value="SBW_NC"/>
<element name="JP3" library="jumper" package="JP1M" value="GND"/>
<element name="U$4" library="LP_Silkscreen" package="MS_TM" value="MS_TM"/>
<element name="U$3" library="LP_Silkscreen" package="5529_REAR_SILK_REV1_5_FINAL" value="5529_REAR_SILK_REV1_5_FINAL"/>
<element name="LED1" library="led" package="CHIP-LED0603" value=""/>
<element name="LED2" library="led" package="CHIP-LED0603" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C18" pad="1"/>
<contactref element="J10" pad="1"/>
<contactref element="J10" pad="2"/>
<contactref element="J1" pad="4"/>
<contactref element="J5" pad="2"/>
<contactref element="C101" pad="2"/>
<contactref element="C102" pad="2"/>
<contactref element="C103" pad="2"/>
<contactref element="C104" pad="-"/>
<contactref element="C107" pad="2"/>
<contactref element="LED101" pad="C"/>
<contactref element="LED102" pad="C"/>
<contactref element="C112" pad="2"/>
<contactref element="R122" pad="2"/>
<contactref element="C122" pad="1"/>
<contactref element="R125" pad="2"/>
<contactref element="C123" pad="1"/>
<contactref element="C121" pad="2"/>
<contactref element="MSP101" pad="56"/>
<contactref element="MSP101" pad="49"/>
<contactref element="MSP101" pad="TP"/>
<contactref element="MSP101" pad="14"/>
<contactref element="MSP101" pad="16"/>
<contactref element="MSP101" pad="39"/>
<contactref element="Q101" pad="2"/>
<contactref element="C113" pad="2"/>
<contactref element="C404" pad="1"/>
<contactref element="U402" pad="1"/>
<contactref element="U402" pad="4"/>
<contactref element="C401" pad="1"/>
<contactref element="Q401" pad="2"/>
<contactref element="J401" pad="GND"/>
<contactref element="U404" pad="4"/>
<contactref element="IC401" pad="28"/>
<contactref element="IC401" pad="27"/>
<contactref element="IC401" pad="31"/>
<contactref element="C16" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="Q4" pad="2"/>
<contactref element="R106" pad="1"/>
<contactref element="C402" pad="2"/>
<contactref element="C405" pad="2"/>
<contactref element="R414" pad="2"/>
<contactref element="C410" pad="2"/>
<contactref element="C411" pad="2"/>
<contactref element="R401" pad="2"/>
<contactref element="C403" pad="-"/>
<contactref element="TP104" pad="1"/>
<contactref element="C408" pad="2"/>
<contactref element="C406" pad="2"/>
<contactref element="IC401" pad="7"/>
<contactref element="C407" pad="2"/>
<contactref element="C409" pad="2"/>
<contactref element="R415" pad="2"/>
<contactref element="R418" pad="2"/>
<contactref element="R419" pad="2"/>
<contactref element="C412" pad="2"/>
<contactref element="R412" pad="1"/>
<contactref element="R409" pad="1"/>
<contactref element="R408" pad="1"/>
<contactref element="R413" pad="1"/>
<contactref element="C111" pad="2"/>
<contactref element="C110" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="S3" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="U6" pad="68"/>
<contactref element="C27" pad="-"/>
<contactref element="U6" pad="61"/>
<contactref element="C26" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="U6" pad="14"/>
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="-"/>
<contactref element="C19" pad="1"/>
<contactref element="U6" pad="19"/>
<contactref element="C14" pad="2"/>
<contactref element="U6" pad="49"/>
<contactref element="S1" pad="2"/>
<contactref element="S2" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C21" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="Q2" pad="P3"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="RST/SBWTDIO">
<contactref element="U6" pad="76"/>
<contactref element="J5" pad="10"/>
<contactref element="C17" pad="1"/>
<contactref element="R27" pad="1"/>
<contactref element="S3" pad="2"/>
<contactref element="JP4.2" pad="2"/>
</signal>
<signal name="TEST/SBWTCK">
<contactref element="U6" pad="71"/>
<contactref element="JP4.1" pad="2"/>
</signal>
<signal name="P1.1">
<contactref element="U6" pad="22"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="P1.2">
<contactref element="U6" pad="23"/>
<contactref element="J5" pad="11"/>
</signal>
<signal name="+5V">
<contactref element="U6" pad="65"/>
<contactref element="C27" pad="+"/>
<contactref element="JP1" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="C28" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="P1.4">
<contactref element="U6" pad="25"/>
<contactref element="J5" pad="7"/>
</signal>
<signal name="P2.6">
<contactref element="U6" pad="35"/>
<contactref element="J5" pad="16"/>
</signal>
<signal name="P1.3">
<contactref element="U6" pad="24"/>
<contactref element="J5" pad="9"/>
</signal>
<signal name="P3.2">
<contactref element="U6" pad="39"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="P1.5">
<contactref element="U6" pad="26"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="P1.7">
<contactref element="U6" pad="28"/>
<contactref element="JP6.3" pad="2"/>
</signal>
<signal name="TARGET_PUR">
<contactref element="U6" pad="63"/>
<contactref element="R16" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="V18">
<contactref element="C15" pad="1"/>
<contactref element="U6" pad="67"/>
</signal>
<signal name="P5.2/XT2IN">
<contactref element="U6" pad="69"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="P5.3/XT2OUT">
<contactref element="U6" pad="70"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R29" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$35">
<contactref element="R30" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="P1.0">
<contactref element="U6" pad="21"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="VCORE">
<contactref element="C18" pad="2"/>
<contactref element="U6" pad="20"/>
</signal>
<signal name="P5.4/XIN">
<contactref element="U6" pad="12"/>
<contactref element="C26" pad="2"/>
<contactref element="Q2" pad="P2"/>
</signal>
<signal name="P5.5/XOUT">
<contactref element="U6" pad="13"/>
<contactref element="C25" pad="2"/>
<contactref element="Q2" pad="P1"/>
</signal>
<signal name="P6.2">
<contactref element="U6" pad="79"/>
<contactref element="J1" pad="10"/>
</signal>
<signal name="P1.6">
<contactref element="U6" pad="27"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="P6.4">
<contactref element="U6" pad="1"/>
<contactref element="J1" pad="14"/>
</signal>
<signal name="P6.3">
<contactref element="U6" pad="80"/>
<contactref element="J1" pad="12"/>
</signal>
<signal name="P6.1">
<contactref element="U6" pad="78"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="AVCC">
<contactref element="R28" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="U6" pad="11"/>
</signal>
<signal name="P6.6">
<contactref element="U6" pad="3"/>
<contactref element="J1" pad="11"/>
</signal>
<signal name="P6.7">
<contactref element="U6" pad="4"/>
<contactref element="JP6.4" pad="2"/>
</signal>
<signal name="P2.0">
<contactref element="U6" pad="29"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="P4.7">
<contactref element="U6" pad="54"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="P3.4">
<contactref element="U6" pad="41"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="P2.5">
<contactref element="U6" pad="34"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="P3.3">
<contactref element="U6" pad="40"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="P2.7">
<contactref element="U6" pad="36"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="P6.0">
<contactref element="U6" pad="77"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="P2.4">
<contactref element="U6" pad="33"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="P2.3">
<contactref element="U6" pad="32"/>
<contactref element="J5" pad="18"/>
</signal>
<signal name="P2.1">
<contactref element="U6" pad="30"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="P2.2">
<contactref element="U6" pad="31"/>
<contactref element="J5" pad="6"/>
</signal>
<signal name="P3.7">
<contactref element="U6" pad="44"/>
<contactref element="J5" pad="17"/>
</signal>
<signal name="P4.0">
<contactref element="U6" pad="45"/>
<contactref element="J5" pad="15"/>
</signal>
<signal name="P6.5">
<contactref element="U6" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="P4.4/UCA1TXD">
<contactref element="U6" pad="51"/>
<contactref element="JP6.1" pad="2"/>
</signal>
<signal name="P4.5/UCA1RXD">
<contactref element="U6" pad="52"/>
<contactref element="JP6.2" pad="2"/>
</signal>
<signal name="P3.6">
<contactref element="U6" pad="43"/>
<contactref element="J1" pad="18"/>
</signal>
<signal name="P4.1">
<contactref element="U6" pad="46"/>
<contactref element="J1" pad="19"/>
</signal>
<signal name="P3.0">
<contactref element="U6" pad="37"/>
<contactref element="J5" pad="12"/>
</signal>
<signal name="P3.1">
<contactref element="U6" pad="38"/>
<contactref element="J5" pad="14"/>
</signal>
<signal name="P3.5">
<contactref element="U6" pad="42"/>
<contactref element="J1" pad="20"/>
</signal>
<signal name="P4.2">
<contactref element="U6" pad="47"/>
<contactref element="J1" pad="17"/>
</signal>
<signal name="P4.3">
<contactref element="U6" pad="48"/>
<contactref element="J5" pad="13"/>
</signal>
<signal name="N$7">
<contactref element="JP8" pad="2"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="EZFET_LED0">
<contactref element="R101" pad="2"/>
<contactref element="MSP101" pad="20"/>
</signal>
<signal name="EZFET_LED1">
<contactref element="R102" pad="2"/>
<contactref element="MSP101" pad="21"/>
</signal>
<signal name="N$1">
<contactref element="R101" pad="1"/>
<contactref element="LED101" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R102" pad="1"/>
<contactref element="LED102" pad="A"/>
</signal>
<signal name="EZFET_AVBUS">
<contactref element="R124" pad="2"/>
<contactref element="R125" pad="1"/>
<contactref element="C123" pad="2"/>
<contactref element="MSP101" pad="1"/>
</signal>
<signal name="EZFET_RST">
<contactref element="MSP101" pad="64"/>
<contactref element="C112" pad="1"/>
<contactref element="R109" pad="1"/>
<contactref element="TP110" pad="1"/>
</signal>
<signal name="EZFET_TCK">
<contactref element="MSP101" pad="63"/>
<contactref element="TP109" pad="1"/>
</signal>
<signal name="EZFET_TMS">
<contactref element="MSP101" pad="62"/>
<contactref element="TP108" pad="1"/>
</signal>
<signal name="EZFET_TDI">
<contactref element="MSP101" pad="61"/>
<contactref element="TP107" pad="1"/>
</signal>
<signal name="EZFET_TDO">
<contactref element="MSP101" pad="60"/>
<contactref element="TP106" pad="1"/>
</signal>
<signal name="EZFET_TEST">
<contactref element="MSP101" pad="59"/>
<contactref element="TP105" pad="1"/>
</signal>
<signal name="EZFET_XT2OUT">
<contactref element="MSP101" pad="58"/>
<contactref element="Q101" pad="3"/>
</signal>
<signal name="EZFET_XT2IN">
<contactref element="MSP101" pad="57"/>
<contactref element="Q101" pad="1"/>
</signal>
<signal name="EZFET_V18">
<contactref element="MSP101" pad="55"/>
<contactref element="C102" pad="1"/>
</signal>
<signal name="EZFET_VUSB">
<contactref element="MSP101" pad="54"/>
<contactref element="C107" pad="1"/>
</signal>
<signal name="EZFET_PUR">
<contactref element="MSP101" pad="51"/>
<contactref element="R105" pad="2"/>
</signal>
<signal name="EZFET_VREF">
<contactref element="C121" pad="1"/>
<contactref element="MSP101" pad="9"/>
</signal>
<signal name="EZFET_UARTRTS">
<contactref element="MSP101" pad="33"/>
<contactref element="JP6.3" pad="1"/>
</signal>
<signal name="EZFET_AVCCOUT2ADC">
<contactref element="R121" pad="2"/>
<contactref element="R122" pad="1"/>
<contactref element="C122" pad="2"/>
<contactref element="MSP101" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="J401" pad="SHIELD1"/>
<contactref element="R401" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J401" pad="D+"/>
<contactref element="U404" pad="5"/>
<contactref element="R405" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="J401" pad="D-"/>
<contactref element="U404" pad="3"/>
<contactref element="R406" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="IC401" pad="2"/>
<contactref element="C406" pad="1"/>
<contactref element="R406" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC401" pad="1"/>
<contactref element="R403" pad="2"/>
<contactref element="R405" pad="1"/>
<contactref element="C405" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="R416" pad="1"/>
<contactref element="C412" pad="1"/>
<contactref element="IC401" pad="11"/>
</signal>
<signal name="N$17">
<contactref element="R417" pad="1"/>
<contactref element="C411" pad="1"/>
<contactref element="IC401" pad="12"/>
</signal>
<signal name="N$18">
<contactref element="R411" pad="1"/>
<contactref element="C409" pad="1"/>
<contactref element="IC401" pad="16"/>
</signal>
<signal name="N$3">
<contactref element="R410" pad="1"/>
<contactref element="C410" pad="1"/>
<contactref element="IC401" pad="15"/>
</signal>
<signal name="TARGET_DP">
<contactref element="U6" pad="62"/>
<contactref element="R32" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="TARGET_DM">
<contactref element="U6" pad="64"/>
<contactref element="R31" pad="2"/>
<contactref element="C24" pad="1"/>
</signal>
<signal name="!PWRON">
<contactref element="IC401" pad="9"/>
<contactref element="IC401" pad="13"/>
<contactref element="IC401" pad="17"/>
<contactref element="IC401" pad="21"/>
</signal>
<signal name="!OC">
<contactref element="IC401" pad="10"/>
<contactref element="IC401" pad="14"/>
<contactref element="IC401" pad="18"/>
<contactref element="IC401" pad="22"/>
<contactref element="R402" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="S5" pad="2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="EZFET_VCC">
<contactref element="MSP101" pad="15"/>
<contactref element="MSP101" pad="11"/>
<contactref element="C113" pad="1"/>
<contactref element="C104" pad="+"/>
<contactref element="R109" pad="2"/>
<contactref element="MSP101" pad="40"/>
<contactref element="C103" pad="1"/>
<contactref element="R121" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="U402" pad="6"/>
<contactref element="C401" pad="2"/>
<contactref element="L401" pad="P$2"/>
<contactref element="R403" pad="1"/>
<contactref element="R404" pad="1"/>
<contactref element="IC401" pad="26"/>
<contactref element="IC401" pad="25"/>
<contactref element="IC401" pad="3"/>
<contactref element="IC401" pad="6"/>
<contactref element="IC401" pad="8"/>
<contactref element="C407" pad="1"/>
<contactref element="R402" pad="1"/>
</signal>
<signal name="EZFET_VBUS">
<contactref element="MSP101" pad="53"/>
<contactref element="R124" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="J401" pad="VBUS"/>
<contactref element="U404" pad="1"/>
<contactref element="C402" pad="1"/>
<contactref element="C403" pad="+"/>
<contactref element="C404" pad="2"/>
<contactref element="U402" pad="3"/>
<contactref element="U402" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="MSP101" pad="17"/>
<contactref element="C101" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U402" pad="2"/>
<contactref element="L401" pad="P$1"/>
</signal>
<signal name="N$15">
<contactref element="R407" pad="2"/>
<contactref element="IC401" pad="29"/>
</signal>
<signal name="N$19">
<contactref element="C408" pad="1"/>
<contactref element="R404" pad="2"/>
<contactref element="IC401" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="IC401" pad="24"/>
<contactref element="R408" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="R409" pad="2"/>
<contactref element="IC401" pad="23"/>
</signal>
<signal name="N$20">
<contactref element="R412" pad="2"/>
<contactref element="IC401" pad="20"/>
</signal>
<signal name="N$23">
<contactref element="IC401" pad="19"/>
<contactref element="R413" pad="2"/>
</signal>
<signal name="HUB_DP2">
<contactref element="R411" pad="2"/>
<contactref element="R104" pad="1"/>
<contactref element="R414" pad="1"/>
</signal>
<signal name="HUB_DM2">
<contactref element="R103" pad="1"/>
<contactref element="R410" pad="2"/>
<contactref element="R415" pad="1"/>
</signal>
<signal name="HUB_DM1">
<contactref element="R31" pad="1"/>
<contactref element="R416" pad="2"/>
<contactref element="R419" pad="1"/>
</signal>
<signal name="HUB_DP1">
<contactref element="R417" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="R418" pad="1"/>
</signal>
<signal name="EZFET_UARTTXD">
<contactref element="MSP101" pad="37"/>
<contactref element="JP6.2" pad="1"/>
</signal>
<signal name="EZFET_UARTRXD">
<contactref element="MSP101" pad="38"/>
<contactref element="JP6.1" pad="1"/>
</signal>
<signal name="EZFET_SBW_RST">
<contactref element="MSP101" pad="43"/>
<contactref element="JP4.2" pad="1"/>
</signal>
<signal name="EZFET_SBW_TST">
<contactref element="MSP101" pad="44"/>
<contactref element="JP4.1" pad="1"/>
</signal>
<signal name="EZFET_UARTCTS">
<contactref element="MSP101" pad="32"/>
<contactref element="JP6.4" pad="1"/>
</signal>
<signal name="EZFET_PU.1/DM">
<contactref element="MSP101" pad="52"/>
<contactref element="C110" pad="1"/>
<contactref element="R103" pad="2"/>
</signal>
<signal name="EZFET_PU.0/DP">
<contactref element="MSP101" pad="50"/>
<contactref element="R105" pad="1"/>
<contactref element="R106" pad="2"/>
<contactref element="R104" pad="2"/>
<contactref element="C111" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="R28" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="S5" pad="1"/>
<contactref element="C30" pad="+"/>
<contactref element="U6" pad="18"/>
<contactref element="C19" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="U6" pad="50"/>
<contactref element="JP2" pad="2"/>
<contactref element="J10" pad="3"/>
<contactref element="J1" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R407" pad="1"/>
<contactref element="Q401" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="Q401" pad="1"/>
<contactref element="IC401" pad="30"/>
</signal>
<signal name="N$9">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$26">
</signal>
<signal name="N$27">
</signal>
<signal name="N$29">
</signal>
<signal name="N$30">
</signal>
<signal name="N$31">
</signal>
<signal name="N$33">
</signal>
<signal name="N$34">
</signal>
<signal name="TARGET_VUSB">
<contactref element="C16" pad="1"/>
<contactref element="U6" pad="66"/>
</signal>
<signal name="EZFET_SBW_NC">
<contactref element="MSP101" pad="45"/>
<contactref element="JP4.3" pad="1"/>
</signal>
<signal name="P7.4">
<contactref element="U6" pad="57"/>
<contactref element="J5" pad="8"/>
</signal>
<signal name="P7.0">
<contactref element="J1" pad="16"/>
<contactref element="U6" pad="5"/>
</signal>
<signal name="P8.1">
<contactref element="U6" pad="16"/>
<contactref element="J5" pad="20"/>
</signal>
<signal name="P8.2">
<contactref element="U6" pad="17"/>
<contactref element="J5" pad="19"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
