| 9.5 |  | Port Address Translation (PAT) |
| 9.5.3 |  | Mapping subnets to PAT addresses |

| With software versions 5.2 and higher, administrators can specify multiple PATs to track use among different subnets. The figure shows that network 10.0.1.0 and network 10.0.2.0 are mapped to different PAT addresses. Using a separate nat and global command pair for each network does this. Outbound sessions from hosts on internal network 10.0.1.0 will appear to originate from address 192.168.0.8, and outbound sessions from hosts on internal network 10.0.2.0 will appear to originate from address 192.168.0.9.