Modules: | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | All |

Module 13: PIX Failover and System Maintenance

Module Overview |
13.1 | Understanding Failover

13.1.1 | PIX Security Appliance failover overview
13.1.2 | IP addresses for failover
13.1.3 | Configuration replication
13.1.4 | Failover and stateful failover
13.1.5 | Failover interface tests

13.2 | Serial Cable Failover Configuration

13.2.1 | Overview of configuring serial cable failover
13.2.2 | Steps 1-4 configuring serial cable failover
13.2.3 | Additional failover commands
13.2.4 | Verifying failover configuration

13.3 | LAN-Based Failover

13.3.1 | LAN-based failover overview
13.3.2 | Steps 1-4: preparing the primary PIX Security Appliance
13.3.3 | Steps 5-10: Preparing the secondary PIX Security Appliance

13.4 | System Maintenance via Remote Access

13.4.1 | Configuring telnet access to the PIX Security Appliance console
13.4.2 | SSH connections to the PIX Security Appliance
13.4.3 | Connecting to the PIX Security Appliance with an SSH client

13.5 | Command Authorization

13.5.1 | Command authorization overview
13.5.2 | (Method 1) enable level command authorization
13.5.3 | (Method 2) local command authorization
13.5.4 | (Method 3) ACS command authorization

13.6 | PIX Security Appliance Password Recovery and Upgrades

13.6.1 | Password Recovery
13.6.2 | Upgrading the image and the activation key

Module Summary |
Module Quiz |

| Close Window |

| All contents copyright © 2002 Cisco Systems, Inc. All rights reserved.