Modules: | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | All |

Module 11: PIX Security Appliance AAA

Module Overview |
11.1 | AAA

11.1.1 | Overview of authentication, authorization, and accounting
11.1.2 | What the user sees
11.1.3 | Cut-through proxy operation
11.1.4 | TACACS+ and RADIUS
11.1.5 | Cisco Secure ACS and the PIX Security Appliance

11.2 | Authentication Configuration

11.2.1 | Configuring the PIX Security Appliance to support authentication
11.2.2 | AAA authentication example
11.2.3 | Authentication of non-Telnet, FTP, or HTTP traffic
11.2.4 | Virtual Telnet
11.2.5 | Virtual HTTP
11.2.6 | Authentication of console access
11.2.7 | Changing authentication timeouts and authentication prompts

11.3 | Authorization and Accounting Configuration

11.3.1 | Configuring the PIX Security Appliance to support AAA authorization
11.3.2 | Providing authorization using downloadable ACLs
11.3.3 | Configuring the PIX Security Appliance to support AAA accounting
11.3.4 | Defining traffic to utilize AAA services
11.3.5 | Monitoring the AAA configuration

11.4 | PPPoE and the PIX Security Appliance

11.4.1 | Overview of PPPoE
11.4.2 | The PIX Security Appliance and PPPoE
11.4.3 | Configuring the PIX Security Appliance to support PPPoE
11.4.4 | Monitoring and troubleshooting the PPPoE client

Module Summary |
Module Quiz |

| Close Window |

| All contents copyright © 2002 Cisco Systems, Inc. All rights reserved.