| 7.4 |  | VPN Enterprise Management |
| 7.4.5 |  | Installation process |

| The Router MC is automatically installed in the CiscoWorks Common Services installation folder. The default folder location is C:\Program Files\CSCOpx\MDC\iosmdc, where C:\ is the drive of installation. A typical installation of the Router MC takes approximately ten minutes.

Complete the following steps to install the Router MC:

1. Insert the Cisco Router MC CD into the CD-ROM drive. If autorun is enabled, the CD should start the installation process automatically. If autorun is not enabled, locate the setup.exe file on the CD-ROM and execute it.
2. The Extracting Files dialog box appears. After the progress bar indicates that all appears files have been extracted, the InstallShield Wizard preparation dialog box appears.
3. Click Next. The Router MC Installation window displays, requesting a password for the Router MC database.
4. Enter a password in the Password field, and confirm the password in the Confirm Password field.
5. Click Next. The Start Copying Files window is displayed.
6. Click Next. The Setup Status window is displayed with an installation status bar that shows the installation progress. After the installation completes, the InstallShield Wizard Complete window is displayed.
7. Select the Yes, I want to restart my computer now radio button, and click Finish. The computer will restart to complete the installation of the Router MC.