| 14.5 |  | Task 3 - Configure IPSec Parameters |
| 14.5.2 |  | Example crypto ACLs |

| Use the show access-list command to display the currently configured ACLs. Figure contains an example ACL for each of the peer PIX Security Appliances. Each PIX Security Appliance in this example has a static mapping of a global IP address to an inside host. The ACL source field is configured for the global IP address of a static translation. The destination field is the global IP address of the peer PIX Security Appliance. The ACLs must be symmetrical to work properly.