| 7.3 |  | Cisco VPN 3.5 Client |
| 7.3.3 |  | Working with the Cisco VPN 3.5 Client |

| This section contains information regarding the VPN Client program menus, log viewer, and status displays. Figure displays the VPN Client program menu as viewed on a Windows 2000 PC. After the VPN Client is installed, access the VPN Client program menu by choosing Start > Programs > Cisco Systems VPN Client. Under the VPN Client menu, the following options are available:

- Certificate Manager - Enables administrators to enroll, import, export, verify, and view certificates.
- Help - Accesses VPN Client help text. Help is also available by doing any of the following:

- Press F1 at any window while using the VPN Client.
- Click the Help button on windows that display it.
- Click on the logo in the title bar.

- Log Viewer - Displays the VPN Client event log.
- Set MTU - The VPN Client automatically sets the MTU size to approximately 1420 bytes. For unique applications, Set MTU can change the MTU size to fit a specific scenario.
- Uninstall VPN Client - Only one VPN Client can be loaded at a time. When upgrading, the old VPN Client must be uninstalled before the new VPN Client is installed. Choose Uninstall VPN Client to remove the old VPN Client.
- VPN Dialer - Initiates the VPN Client connection process by displaying the VPN Client splash window.