Modules: | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 | All |

Module 8: PIX Security Appliance

Module Overview |
8.1 | Introduction to Firewalls

8.1.1 | Firewalls and firewall technologies
8.1.2 | Firewall technologies
8.1.3 | The firewall marketplace
8.1.4 | Security and VPN certifications

8.2 | The Cisco PIX Security Appliance

8.2.1 | Introduction to the PIX Security Appliance
8.2.2 | The Finesse operating system
8.2.3 | Adaptive Security Algorithm (ASA)
8.2.4 | Cut-through proxy operation
8.2.5 | Failover
8.2.6 | Network Address Translation (NAT)
8.2.7 | The PIX Security Appliance family
8.2.8 | Firewall Services Module (FWSM)
8.2.9 | License types and VPN capabilities

8.3 | Getting Started

8.3.1 | User interface
8.3.2 | Basic PIX Security Appliance configurations commands
8.3.3 | Examine PIX Security Appliance status

8.4 | Routing and Multicast Configuration

8.4.1 | Static routes
8.4.2 | Dynamic routes
8.4.3 | Multicast routing
8.4.4 | Allowing hosts to receive multicast transmissions
8.4.5 | Forwarding multicasts from a transmission source
8.4.6 | View and debug SMR

8.5 | PIX Dynamic Host Configuration Protocol (DHCP)

8.5.1 | Sever and client
8.5.2 | DHCP server
8.5.3 | Configuring the PIX Security Appliance as a DHCP server

Module Summary |
Module Quiz |

| Close Window |

| All contents copyright © 2002 Cisco Systems, Inc. All rights reserved.