<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.2">
<drawing>
<library>
<description>&lt;b&gt;TTL Devices with DIN Symbols&lt;/b&gt;&lt;p&gt;
CadSoft and the author do not warrant that this library is free from error
or will meet your specific requirements.&lt;p&gt;
&lt;author&gt;Created by Holger Bettenbühl, hol.bet.@rhein-main.net&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL20">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="DIL24-3">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.3 inch</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="+UB">
<pin name="+UB" direction="pwr"/>
</symbol>
<symbol name="-UB">
<pin name="-UB" direction="pwr"/>
</symbol>
<symbol name="32">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="00">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="02">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="86">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="11">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="21">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="04">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="133">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="I" direction="in"/>
<pin name="J" direction="in"/>
<pin name="K" direction="in"/>
<pin name="L" direction="in"/>
<pin name="M" direction="in"/>
</symbol>
<symbol name="10">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="20">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="30">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
</symbol>
<symbol name="27">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="05">
<pin name="A" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="09">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="14">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="42">
<pin name="Y4" direction="out"/>
<pin name="D" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="Y8" direction="out"/>
<pin name="Y9" direction="out"/>
</symbol>
<symbol name="51_2">
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="51_1">
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="73">
<pin name="CLK" direction="in"/>
<pin name="J" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="K" direction="in"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="74">
<pin name="CLK" direction="in"/>
<pin name="!PRE" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="75">
<pin name="1D" direction="in"/>
<pin name="1Q" direction="out"/>
<pin name="2D" direction="in"/>
<pin name="1C,2C" direction="in"/>
<pin name="!1Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="!2Q" direction="out"/>
</symbol>
<symbol name="76">
<pin name="!PRE" direction="in"/>
<pin name="J" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="K" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="77">
<pin name="1D" direction="in"/>
<pin name="1Q" direction="out"/>
<pin name="2D" direction="in"/>
<pin name="1C,2C" direction="in"/>
<pin name="2Q" direction="out"/>
</symbol>
<symbol name="78">
<pin name="CLK" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!1PRE" direction="in"/>
<pin name="!2PRE" direction="in"/>
<pin name="!1Q" direction="out"/>
<pin name="!2Q" direction="out"/>
<pin name="1J" direction="in"/>
<pin name="1K" direction="in"/>
<pin name="2J" direction="in"/>
<pin name="2K" direction="in"/>
<pin name="1Q" direction="out"/>
<pin name="2Q" direction="out"/>
</symbol>
<symbol name="85A">
<pin name="Q3" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="Q1" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="PGTQ_" direction="in"/>
<pin name="PEQQ_" direction="in"/>
<pin name="PLTQ_" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="PLTQ" direction="out"/>
<pin name="PEQQ" direction="out"/>
<pin name="PGTQ" direction="out"/>
</symbol>
<symbol name="109">
<pin name="!PRE" direction="in"/>
<pin name="J" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
<pin name="!K" direction="in"/>
<pin name="CLK" direction="in"/>
</symbol>
<symbol name="113">
<pin name="CLK" direction="in"/>
<pin name="J" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!PRE" direction="in"/>
<pin name="K" direction="in"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="125">
<pin name="!G" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y" direction="hiz"/>
</symbol>
<symbol name="132">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="137">
<pin name="Y7" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="!G2" direction="in"/>
<pin name="!GL" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="138">
<pin name="Y7" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="!G2A" direction="in"/>
<pin name="!G2B" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="139">
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="!G" direction="in"/>
</symbol>
<symbol name="147">
<pin name="9" direction="in"/>
<pin name="8" direction="in"/>
<pin name="7" direction="in"/>
<pin name="6" direction="in"/>
<pin name="5" direction="in"/>
<pin name="4" direction="in"/>
<pin name="3" direction="in"/>
<pin name="2" direction="in"/>
<pin name="1" direction="in"/>
<pin name="A" direction="out"/>
<pin name="B" direction="out"/>
<pin name="C" direction="out"/>
<pin name="D" direction="out"/>
</symbol>
<symbol name="148">
<pin name="EI" direction="in"/>
<pin name="A2" direction="out"/>
<pin name="A1" direction="out"/>
<pin name="A0" direction="out"/>
<pin name="7" direction="in"/>
<pin name="6" direction="in"/>
<pin name="5" direction="in"/>
<pin name="4" direction="in"/>
<pin name="3" direction="in"/>
<pin name="2" direction="in"/>
<pin name="1" direction="in"/>
<pin name="0" direction="in"/>
<pin name="GS" direction="out"/>
<pin name="EO" direction="out"/>
</symbol>
<symbol name="151">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="W" direction="out"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="152">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="W" direction="out"/>
</symbol>
<symbol name="01">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="154">
<pin name="15" direction="out"/>
<pin name="14" direction="out"/>
<pin name="13" direction="out"/>
<pin name="12" direction="out"/>
<pin name="11" direction="out"/>
<pin name="10" direction="out"/>
<pin name="9" direction="out"/>
<pin name="8" direction="out"/>
<pin name="7" direction="out"/>
<pin name="6" direction="out"/>
<pin name="5" direction="out"/>
<pin name="4" direction="out"/>
<pin name="3" direction="out"/>
<pin name="2" direction="out"/>
<pin name="1" direction="out"/>
<pin name="0" direction="out"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="157">
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="!A!/B" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="4Y" direction="out"/>
</symbol>
<symbol name="160">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="ENT" direction="in"/>
<pin name="!LOAD" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="164">
<pin name="QH" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!CLR" direction="in"/>
</symbol>
<symbol name="165">
<pin name="SH/!LD" direction="in"/>
<pin name="CLK_INH" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="QH" direction="out"/>
<pin name="!QH" direction="out"/>
</symbol>
<symbol name="166">
<pin name="SH/!LD" direction="in"/>
<pin name="CLK_INH" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SER" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="QH" direction="out"/>
<pin name="!CLR" direction="in"/>
</symbol>
<symbol name="173">
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="1Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="CLK" direction="in"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="N" direction="in"/>
<pin name="M" direction="in"/>
<pin name="CLR" direction="in"/>
</symbol>
<symbol name="174">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="6Q" direction="out"/>
<pin name="5Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="1Q" direction="out"/>
</symbol>
<symbol name="175">
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!4Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="!3Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="!2Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="!1Q" direction="out"/>
<pin name="1Q" direction="out"/>
</symbol>
<symbol name="180">
<pin name="H" direction="in"/>
<pin name="G" direction="in"/>
<pin name="F" direction="in"/>
<pin name="E" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="ODD" direction="in"/>
<pin name="EVEN" direction="in"/>
<pin name="SEVEN" direction="out"/>
<pin name="SODD" direction="out"/>
</symbol>
<symbol name="190">
<pin name="!LOAD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="D/!U" direction="in"/>
<pin name="!CTEN" direction="in"/>
<pin name="!RCO" direction="out"/>
<pin name="MAX/MIN" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="192">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="!LOAD" direction="in"/>
<pin name="UP" direction="in"/>
<pin name="CLR" direction="in"/>
<pin name="!CO" direction="out"/>
<pin name="DOWN" direction="in"/>
<pin name="!BO" direction="out"/>
</symbol>
<symbol name="194">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="S1" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="SR_SER" direction="in"/>
<pin name="SL_SER" direction="in"/>
</symbol>
<symbol name="195">
<pin name="SH/!LD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="J" direction="in"/>
<pin name="!K" direction="in"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!QD" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
</symbol>
<symbol name="08">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="03">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="107">
<pin name="CLK" direction="in"/>
<pin name="J" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="K" direction="in"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="112">
<pin name="!PRE" direction="in"/>
<pin name="J" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="K" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="114">
<pin name="CLK" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="!1PRE" direction="in"/>
<pin name="!2PRE" direction="in"/>
<pin name="!1Q" direction="out"/>
<pin name="!2Q" direction="out"/>
<pin name="1J" direction="in"/>
<pin name="1K" direction="in"/>
<pin name="2J" direction="in"/>
<pin name="2K" direction="in"/>
<pin name="1Q" direction="out"/>
<pin name="2Q" direction="out"/>
</symbol>
<symbol name="36">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="126">
<pin name="G" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y" direction="hiz"/>
</symbol>
<symbol name="162">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="ENT" direction="in"/>
<pin name="!LOAD" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="191">
<pin name="!LOAD" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="D/!U" direction="in"/>
<pin name="!CTEN" direction="in"/>
<pin name="!RCO" direction="out"/>
<pin name="MAX/MIN" direction="out"/>
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="193">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="!LOAD" direction="in"/>
<pin name="UP" direction="in"/>
<pin name="CLR" direction="in"/>
<pin name="!CO" direction="out"/>
<pin name="DOWN" direction="in"/>
<pin name="!BO" direction="out"/>
</symbol>
<symbol name="161">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="ENT" direction="in"/>
<pin name="!LOAD" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="163">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="ENP" direction="in"/>
<pin name="ENT" direction="in"/>
<pin name="!LOAD" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="RCO" direction="out"/>
</symbol>
<symbol name="153">
<pin name="2C3" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C0" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
<pin name="!1G" direction="in"/>
<pin name="!2G" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="158">
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="!A!/B" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="3Y" direction="out"/>
<pin name="4Y" direction="out"/>
</symbol>
<symbol name="240">
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="241_1">
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="242">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="G2" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
</symbol>
<symbol name="244">
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="245">
<pin name="A8"/>
<pin name="A7"/>
<pin name="A6"/>
<pin name="A5"/>
<pin name="A4"/>
<pin name="A3"/>
<pin name="DIR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="B8"/>
<pin name="B7"/>
<pin name="B6"/>
<pin name="B5"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="B1"/>
<pin name="B2"/>
</symbol>
<symbol name="251">
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="W" direction="hiz"/>
<pin name="Y" direction="hiz"/>
</symbol>
<symbol name="253">
<pin name="2C3" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C0" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
<pin name="!1G" direction="in"/>
<pin name="!2G" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2Y" direction="hiz"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="266">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="oc"/>
</symbol>
<symbol name="273">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="6Q" direction="out"/>
<pin name="5Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="1Q" direction="out"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="7Q" direction="out"/>
<pin name="8Q" direction="out"/>
</symbol>
<symbol name="280">
<pin name="F" direction="in"/>
<pin name="E" direction="in"/>
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="SEVEN" direction="out"/>
<pin name="SODD" direction="out"/>
<pin name="I" direction="in"/>
</symbol>
<symbol name="283">
<pin name="S4" direction="out"/>
<pin name="S3" direction="out"/>
<pin name="S2" direction="out"/>
<pin name="S1" direction="out"/>
<pin name="B4" direction="in"/>
<pin name="C0" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="C4" direction="out"/>
</symbol>
<symbol name="298">
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="C2" direction="in"/>
<pin name="C1" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="WS" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
</symbol>
<symbol name="299">
<pin name="C/QC" direction="in"/>
<pin name="H/QH" direction="in"/>
<pin name="B/QB" direction="in"/>
<pin name="A/QA" direction="in"/>
<pin name="QA*" direction="out"/>
<pin name="QH*" direction="out"/>
<pin name="S1" direction="in"/>
<pin name="CLK" direction="out"/>
<pin name="S0" direction="in"/>
<pin name="!CLR" direction="in"/>
<pin name="SR" direction="in"/>
<pin name="SL" direction="in"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="D/QD" direction="in"/>
<pin name="E/QE" direction="in"/>
<pin name="F/QF" direction="in"/>
<pin name="G/QG" direction="in"/>
</symbol>
<symbol name="354">
<pin name="!SC" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="G3" direction="in"/>
<pin name="!DC" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="W" direction="hiz"/>
<pin name="Y" direction="hiz"/>
</symbol>
<symbol name="365">
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="366">
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="367_1">
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="368_1">
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="368_2">
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="367_2">
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="374">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OC" direction="in"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="7Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
</symbol>
<symbol name="377">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="6Q" direction="out"/>
<pin name="5Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="1Q" direction="out"/>
<pin name="8D" direction="in"/>
<pin name="7D" direction="in"/>
<pin name="7Q" direction="out"/>
<pin name="8Q" direction="out"/>
</symbol>
<symbol name="378">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="6Q" direction="out"/>
<pin name="5Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="1Q" direction="out"/>
</symbol>
<symbol name="379">
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!4Q" direction="out"/>
<pin name="4Q" direction="out"/>
<pin name="!3Q" direction="out"/>
<pin name="3Q" direction="out"/>
<pin name="!2Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="!1Q" direction="out"/>
<pin name="1Q" direction="out"/>
</symbol>
<symbol name="390">
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLR" direction="in"/>
<pin name="CKA" direction="in"/>
<pin name="CKB" direction="in"/>
</symbol>
<symbol name="393">
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLR" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="373">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="!OC" direction="in"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="7Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
</symbol>
<symbol name="375">
<pin name="1D" direction="in"/>
<pin name="1Q" direction="out"/>
<pin name="2D" direction="in"/>
<pin name="1C,2C" direction="in"/>
<pin name="!1Q" direction="out"/>
<pin name="2Q" direction="out"/>
<pin name="!2Q" direction="out"/>
</symbol>
<symbol name="386">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="259">
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="D" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="Q3" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q0" direction="out"/>
</symbol>
<symbol name="243">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="G2" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
</symbol>
<symbol name="356">
<pin name="!SC" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="G3" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="D7" direction="in"/>
<pin name="D6" direction="in"/>
<pin name="D5" direction="in"/>
<pin name="D4" direction="in"/>
<pin name="D3" direction="in"/>
<pin name="D2" direction="in"/>
<pin name="D1" direction="in"/>
<pin name="D0" direction="in"/>
<pin name="W" direction="hiz"/>
<pin name="Y" direction="hiz"/>
</symbol>
<symbol name="353">
<pin name="2C3" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C0" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
<pin name="!1G" direction="in"/>
<pin name="!2G" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2Y" direction="hiz"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="352">
<pin name="2C3" direction="in"/>
<pin name="2C2" direction="in"/>
<pin name="2C1" direction="in"/>
<pin name="2C0" direction="in"/>
<pin name="1C3" direction="in"/>
<pin name="1C2" direction="in"/>
<pin name="1C1" direction="in"/>
<pin name="1C0" direction="in"/>
<pin name="!1G" direction="in"/>
<pin name="!2G" direction="in"/>
<pin name="1Y" direction="out"/>
<pin name="2Y" direction="out"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="257">
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="!A!/B" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2Y" direction="hiz"/>
<pin name="3Y" direction="hiz"/>
<pin name="4Y" direction="hiz"/>
</symbol>
<symbol name="258">
<pin name="4B" direction="in"/>
<pin name="4A" direction="in"/>
<pin name="3B" direction="in"/>
<pin name="3A" direction="in"/>
<pin name="2B" direction="in"/>
<pin name="2A" direction="in"/>
<pin name="1B" direction="in"/>
<pin name="1A" direction="in"/>
<pin name="A/!B" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="1Y" direction="hiz"/>
<pin name="2Y" direction="hiz"/>
<pin name="3Y" direction="hiz"/>
<pin name="4Y" direction="hiz"/>
</symbol>
<symbol name="238">
<pin name="Y7" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="!G2A" direction="in"/>
<pin name="!G2B" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="237">
<pin name="Y7" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="!G2" direction="in"/>
<pin name="!GL" direction="in"/>
<pin name="G1" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
</symbol>
<symbol name="239">
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="!G" direction="in"/>
</symbol>
<symbol name="241_2">
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="G" direction="in"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
</symbol>
<symbol name="490">
<pin name="QA" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLR" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="SET9" direction="in"/>
</symbol>
<symbol name="4002">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="4075">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="590A">
<pin name="CCK" direction="in"/>
<pin name="RCK" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="!CCKEN" direction="in"/>
<pin name="!RCO" direction="out"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="!CCLR" direction="in"/>
</symbol>
<symbol name="533">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="!OC" direction="in"/>
<pin name="!6Q" direction="hiz"/>
<pin name="!5Q" direction="hiz"/>
<pin name="!4Q" direction="hiz"/>
<pin name="!3Q" direction="hiz"/>
<pin name="!2Q" direction="hiz"/>
<pin name="!1Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="!7Q" direction="hiz"/>
<pin name="!8Q" direction="hiz"/>
</symbol>
<symbol name="534">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OC" direction="in"/>
<pin name="!6Q" direction="hiz"/>
<pin name="!5Q" direction="hiz"/>
<pin name="!4Q" direction="hiz"/>
<pin name="!3Q" direction="hiz"/>
<pin name="!2Q" direction="hiz"/>
<pin name="!1Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="!7Q" direction="hiz"/>
<pin name="!8Q" direction="hiz"/>
</symbol>
<symbol name="540">
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="Y7" direction="hiz"/>
<pin name="Y8" direction="hiz"/>
</symbol>
<symbol name="541">
<pin name="A6" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="!G2" direction="in"/>
<pin name="!G1" direction="in"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y1" direction="hiz"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="Y7" direction="hiz"/>
<pin name="Y8" direction="hiz"/>
</symbol>
<symbol name="594">
<pin name="SRCK" direction="in"/>
<pin name="RCK" direction="in"/>
<pin name="!RCLR" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="!SRCLR" direction="in"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="SER" direction="in"/>
<pin name="QH*" direction="out"/>
</symbol>
<symbol name="4016">
<pin name="C" direction="in"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="4017">
<pin name="Y7" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="!CLKEN" direction="in"/>
<pin name="CLR" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="Y8" direction="out"/>
<pin name="Y9" direction="out"/>
<pin name="CO" direction="out"/>
</symbol>
<symbol name="4020">
<pin name="QJ" direction="out"/>
<pin name="QI" direction="out"/>
<pin name="QH" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="CLR" direction="in"/>
<pin name="QK" direction="out"/>
<pin name="QL" direction="out"/>
<pin name="QM" direction="out"/>
<pin name="QN" direction="out"/>
</symbol>
<symbol name="4024">
<pin name="QG" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="CLR" direction="in"/>
</symbol>
<symbol name="4040">
<pin name="QH" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="QC" direction="out"/>
<pin name="QB" direction="out"/>
<pin name="QA" direction="out"/>
<pin name="CLK" direction="in"/>
<pin name="CLR" direction="in"/>
<pin name="QI" direction="out"/>
<pin name="QJ" direction="out"/>
<pin name="QK" direction="out"/>
<pin name="QL" direction="out"/>
</symbol>
<symbol name="4060">
<pin name="QL" direction="out"/>
<pin name="QJ" direction="out"/>
<pin name="QI" direction="out"/>
<pin name="QH" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLR" direction="in"/>
<pin name="QM" direction="out"/>
<pin name="QN" direction="out"/>
<pin name="!CKO" direction="out"/>
<pin name="CKO" direction="out"/>
<pin name="CKI" direction="in"/>
</symbol>
<symbol name="4078">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
<pin name="E" direction="in"/>
<pin name="F" direction="in"/>
<pin name="G" direction="in"/>
<pin name="H" direction="in"/>
<pin name="W" direction="out"/>
</symbol>
<symbol name="4514">
<pin name="Y7" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="LE" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y8" direction="out"/>
<pin name="Y9" direction="out"/>
<pin name="Y10" direction="out"/>
<pin name="Y11" direction="out"/>
<pin name="Y12" direction="out"/>
<pin name="Y13" direction="out"/>
<pin name="Y14" direction="out"/>
<pin name="Y15" direction="out"/>
<pin name="D" direction="in"/>
<pin name="!G" direction="in"/>
</symbol>
<symbol name="4724">
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="CLR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="D" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S0" direction="in"/>
<pin name="Q3" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q0" direction="out"/>
</symbol>
<symbol name="573">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="!OC" direction="in"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="7Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
</symbol>
<symbol name="574">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OC" direction="in"/>
<pin name="6Q" direction="hiz"/>
<pin name="5Q" direction="hiz"/>
<pin name="4Q" direction="hiz"/>
<pin name="3Q" direction="hiz"/>
<pin name="2Q" direction="hiz"/>
<pin name="1Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="7Q" direction="hiz"/>
<pin name="8Q" direction="hiz"/>
</symbol>
<symbol name="4066">
<pin name="C" direction="in"/>
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
</symbol>
<symbol name="563">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="!OC" direction="in"/>
<pin name="!6Q" direction="hiz"/>
<pin name="!5Q" direction="hiz"/>
<pin name="!4Q" direction="hiz"/>
<pin name="!3Q" direction="hiz"/>
<pin name="!2Q" direction="hiz"/>
<pin name="!1Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="!7Q" direction="hiz"/>
<pin name="!8Q" direction="hiz"/>
</symbol>
<symbol name="564">
<pin name="6D" direction="in"/>
<pin name="5D" direction="in"/>
<pin name="4D" direction="in"/>
<pin name="3D" direction="in"/>
<pin name="2D" direction="in"/>
<pin name="1D" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!OC" direction="in"/>
<pin name="!6Q" direction="hiz"/>
<pin name="!5Q" direction="hiz"/>
<pin name="!4Q" direction="hiz"/>
<pin name="!3Q" direction="hiz"/>
<pin name="!2Q" direction="hiz"/>
<pin name="!1Q" direction="hiz"/>
<pin name="7D" direction="in"/>
<pin name="8D" direction="in"/>
<pin name="!7Q" direction="hiz"/>
<pin name="!8Q" direction="hiz"/>
</symbol>
<symbol name="595">
<pin name="SRCK" direction="in"/>
<pin name="RCK" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="QA" direction="hiz"/>
<pin name="QB" direction="hiz"/>
<pin name="QC" direction="hiz"/>
<pin name="QD" direction="hiz"/>
<pin name="!SRCLR" direction="in"/>
<pin name="QE" direction="hiz"/>
<pin name="QF" direction="hiz"/>
<pin name="QG" direction="hiz"/>
<pin name="QH" direction="hiz"/>
<pin name="SER" direction="in"/>
<pin name="QH*" direction="out"/>
</symbol>
<symbol name="4515">
<pin name="Y7" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y4" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y0" direction="out"/>
<pin name="LE" direction="in"/>
<pin name="C" direction="in"/>
<pin name="B" direction="in"/>
<pin name="A" direction="in"/>
<pin name="Y8" direction="out"/>
<pin name="Y9" direction="out"/>
<pin name="Y10" direction="out"/>
<pin name="Y11" direction="out"/>
<pin name="Y12" direction="out"/>
<pin name="Y13" direction="out"/>
<pin name="Y14" direction="out"/>
<pin name="Y15" direction="out"/>
<pin name="D" direction="in"/>
<pin name="!G" direction="in"/>
</symbol>
<symbol name="4061">
<pin name="QL" direction="out"/>
<pin name="QJ" direction="out"/>
<pin name="QI" direction="out"/>
<pin name="QH" direction="out"/>
<pin name="QG" direction="out"/>
<pin name="QF" direction="out"/>
<pin name="QE" direction="out"/>
<pin name="QD" direction="out"/>
<pin name="CLR" direction="in"/>
<pin name="QM" direction="out"/>
<pin name="QN" direction="out"/>
<pin name="!CKO" direction="out"/>
<pin name="CKO" direction="out"/>
<pin name="CKI" direction="in"/>
</symbol>
<symbol name="7266">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="620">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="GAB" direction="in"/>
<pin name="!GBA" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="623">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="GAB" direction="in"/>
<pin name="!GBA" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="640">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="!G" direction="in"/>
<pin name="DIR" direction="in"/>
</symbol>
<symbol name="645">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="DIR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="643">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="DIR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="B1"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
</symbol>
<symbol name="646">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="DIR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="CBA" direction="in"/>
<pin name="CAB" direction="in"/>
<pin name="SBA" direction="in"/>
<pin name="SAB" direction="in"/>
<pin name="B1"/>
</symbol>
<symbol name="648">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="DIR" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="CBA" direction="in"/>
<pin name="CAB" direction="in"/>
<pin name="SBA" direction="in"/>
<pin name="SAB" direction="in"/>
<pin name="B1"/>
</symbol>
<symbol name="651">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="!GBA" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="CBA" direction="in"/>
<pin name="CAB" direction="in"/>
<pin name="SBA" direction="in"/>
<pin name="SAB" direction="in"/>
<pin name="B1"/>
<pin name="GAB" direction="in"/>
</symbol>
<symbol name="652">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="A1"/>
<pin name="!GBA" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="CBA" direction="in"/>
<pin name="CAB" direction="in"/>
<pin name="SBA" direction="in"/>
<pin name="SAB" direction="in"/>
<pin name="B1"/>
<pin name="GAB" direction="in"/>
</symbol>
<symbol name="679">
<pin name="A12" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="682">
<pin name="Q7" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="!P=Q" direction="out"/>
<pin name="!P&gt;Q" direction="out"/>
<pin name="Q1" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
</symbol>
<symbol name="688">
<pin name="Q7" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="!P=Q" direction="out"/>
<pin name="Q1" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
<pin name="!G" direction="in"/>
</symbol>
<symbol name="7001">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7002">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7032">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7074_3">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7006_2">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="7006_1">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="7006_3">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7006_4">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7006_5">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
</symbol>
<symbol name="7006_6">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="7074_1">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7074_2">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7074_4">
<pin name="CLK" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!Q" direction="out"/>
<pin name="!PRE" direction="in"/>
</symbol>
<symbol name="7074_5">
<pin name="CLK" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!Q" direction="out"/>
<pin name="!PRE" direction="in"/>
</symbol>
<symbol name="7074_6">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="658">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="!GBA" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="GAB" direction="in"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="APO" direction="out"/>
<pin name="BPO" direction="out"/>
<pin name="BPI" direction="in"/>
<pin name="API" direction="in"/>
</symbol>
<symbol name="659">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="!GBA" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="GAB" direction="in"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="APO" direction="out"/>
<pin name="BPO" direction="out"/>
<pin name="BPI" direction="in"/>
<pin name="API" direction="in"/>
</symbol>
<symbol name="664">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="!G" direction="in"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="DIR" direction="in"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="APO" direction="hiz"/>
<pin name="BPO" direction="hiz"/>
<pin name="BPI" direction="in"/>
<pin name="API" direction="in"/>
</symbol>
<symbol name="665">
<pin name="A4"/>
<pin name="A3"/>
<pin name="A2"/>
<pin name="B4"/>
<pin name="B3"/>
<pin name="B2"/>
<pin name="A5"/>
<pin name="A6"/>
<pin name="A7"/>
<pin name="A8"/>
<pin name="B5"/>
<pin name="B6"/>
<pin name="B7"/>
<pin name="B8"/>
<pin name="A1"/>
<pin name="B1"/>
<pin name="APO" direction="hiz"/>
<pin name="BPO" direction="hiz"/>
<pin name="BPI" direction="in"/>
<pin name="API" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="DIR" direction="in"/>
</symbol>
<symbol name="7022">
<pin name="XCAP" direction="pas"/>
<pin name="CLR" direction="in"/>
<pin name="Y4" direction="out"/>
<pin name="Y5" direction="out"/>
<pin name="Y6" direction="out"/>
<pin name="Y7" direction="out"/>
<pin name="!CLKEN" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="!CLROUT" direction="oc"/>
<pin name="Y0" direction="out"/>
<pin name="Y1" direction="out"/>
<pin name="Y2" direction="out"/>
<pin name="Y3" direction="out"/>
<pin name="CO" direction="out"/>
</symbol>
<symbol name="684">
<pin name="Q7" direction="in"/>
<pin name="Q6" direction="in"/>
<pin name="Q5" direction="in"/>
<pin name="Q4" direction="in"/>
<pin name="Q3" direction="in"/>
<pin name="Q2" direction="in"/>
<pin name="P4" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="!P=Q" direction="out"/>
<pin name="!P&gt;Q" direction="out"/>
<pin name="Q1" direction="in"/>
<pin name="Q0" direction="in"/>
<pin name="P5" direction="in"/>
<pin name="P6" direction="in"/>
<pin name="P7" direction="in"/>
</symbol>
<symbol name="677">
<pin name="A12" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
</symbol>
<symbol name="678">
<pin name="A12" direction="in"/>
<pin name="C" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="Y" direction="out"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
</symbol>
<symbol name="680">
<pin name="A12" direction="in"/>
<pin name="C" direction="in"/>
<pin name="P0" direction="in"/>
<pin name="P1" direction="in"/>
<pin name="P2" direction="in"/>
<pin name="P3" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="604">
<pin name="B4" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="B3" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="B2" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="B1" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="SEL_A/!B" direction="in"/>
<pin name="CLK" direction="in"/>
<pin name="Y1" direction="hiz"/>
<pin name="Y2" direction="hiz"/>
<pin name="Y3" direction="hiz"/>
<pin name="Y4" direction="hiz"/>
<pin name="B8" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="B7" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="B6" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="B5" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="Y5" direction="hiz"/>
<pin name="Y6" direction="hiz"/>
<pin name="Y7" direction="hiz"/>
<pin name="Y8" direction="hiz"/>
</symbol>
<symbol name="7008_1">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7008_2">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7008_3">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7008_4">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7008_5">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7008_6">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7008_7">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7008_8">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7075_1">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7075_2">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7075_4">
<pin name="CLK" direction="in"/>
<pin name="!PRE" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="7075_5">
<pin name="CLK" direction="in"/>
<pin name="!PRE" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="7075_3">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7075_6">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7076_1">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7076_2">
<pin name="A" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7076_4">
<pin name="CLK" direction="in"/>
<pin name="!PRE" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="7076_5">
<pin name="CLK" direction="in"/>
<pin name="!PRE" direction="in"/>
<pin name="Q" direction="out"/>
<pin name="!CLR" direction="in"/>
<pin name="D" direction="in"/>
<pin name="!Q" direction="out"/>
</symbol>
<symbol name="7076_3">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="7076_6">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="805">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="808">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="804">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="832">
<pin name="A" direction="in"/>
<pin name="B" direction="in"/>
<pin name="Y" direction="out"/>
</symbol>
<symbol name="P+UB">
<pin name="+UB" direction="sup"/>
</symbol>
<symbol name="P-UB">
<pin name="-UB" direction="sup"/>
</symbol>
<symbol name="4053">
<pin name="11"/>
<pin name="!G" direction="in"/>
<pin name="13"/>
<pin name="12"/>
<pin name="14"/>
<pin name="10"/>
<pin name="1"/>
<pin name="2"/>
<pin name="15"/>
<pin name="9"/>
<pin name="3"/>
<pin name="5"/>
<pin name="4"/>
</symbol>
<symbol name="PWRVCCGNDVEE">
<pin name="VCC" direction="pwr"/>
<pin name="VEE" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74*00" prefix="V">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="00"/>
<gate name="/2" symbol="00"/>
<gate name="/3" symbol="00"/>
<gate name="/4" symbol="00"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
<technology name="HC"/>
<technology name="HCT"/>
<technology name="LS"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*02" prefix="V">
<description>Quad 2-input &lt;b&gt;NOR&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="02"/>
<gate name="/2" symbol="02"/>
<gate name="/3" symbol="02"/>
<gate name="/4" symbol="02"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="2"/>
<connect gate="/1" pin="B" pad="3"/>
<connect gate="/1" pin="Y" pad="1"/>
<connect gate="/2" pin="A" pad="5"/>
<connect gate="/2" pin="B" pad="6"/>
<connect gate="/2" pin="Y" pad="4"/>
<connect gate="/3" pin="A" pad="8"/>
<connect gate="/3" pin="B" pad="9"/>
<connect gate="/3" pin="Y" pad="10"/>
<connect gate="/4" pin="A" pad="11"/>
<connect gate="/4" pin="B" pad="12"/>
<connect gate="/4" pin="Y" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*04" prefix="V">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="04"/>
<gate name="/2" symbol="04"/>
<gate name="/3" symbol="04"/>
<gate name="/4" symbol="04"/>
<gate name="/5" symbol="04"/>
<gate name="/6" symbol="04"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="Y" pad="2"/>
<connect gate="/2" pin="A" pad="3"/>
<connect gate="/2" pin="Y" pad="4"/>
<connect gate="/3" pin="A" pad="5"/>
<connect gate="/3" pin="Y" pad="6"/>
<connect gate="/4" pin="A" pad="9"/>
<connect gate="/4" pin="Y" pad="8"/>
<connect gate="/5" pin="A" pad="11"/>
<connect gate="/5" pin="Y" pad="10"/>
<connect gate="/6" pin="A" pad="13"/>
<connect gate="/6" pin="Y" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*08" prefix="V">
<description>Quad 2-input &lt;b&gt;AND&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="08"/>
<gate name="/2" symbol="08"/>
<gate name="/3" symbol="08"/>
<gate name="/4" symbol="08"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*10" prefix="V">
<description>Triple 3-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="10"/>
<gate name="/2" symbol="10"/>
<gate name="/3" symbol="10"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="C" pad="13"/>
<connect gate="/1" pin="Y" pad="12"/>
<connect gate="/2" pin="A" pad="3"/>
<connect gate="/2" pin="B" pad="4"/>
<connect gate="/2" pin="C" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="C" pad="11"/>
<connect gate="/3" pin="Y" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*01" prefix="V">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; gate, open collector</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="01"/>
<gate name="/2" symbol="01"/>
<gate name="/3" symbol="01"/>
<gate name="/4" symbol="01"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="2"/>
<connect gate="/1" pin="B" pad="3"/>
<connect gate="/1" pin="Y" pad="1"/>
<connect gate="/2" pin="A" pad="5"/>
<connect gate="/2" pin="B" pad="6"/>
<connect gate="/2" pin="Y" pad="4"/>
<connect gate="/3" pin="A" pad="8"/>
<connect gate="/3" pin="B" pad="9"/>
<connect gate="/3" pin="Y" pad="10"/>
<connect gate="/4" pin="A" pad="11"/>
<connect gate="/4" pin="B" pad="12"/>
<connect gate="/4" pin="Y" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*03" prefix="V">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; gate, open collector output</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="03"/>
<gate name="/2" symbol="03"/>
<gate name="/3" symbol="03"/>
<gate name="/4" symbol="03"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*05" prefix="V">
<description>Hex &lt;b&gt;INVERTER&lt;/b&gt;, open collector</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="05"/>
<gate name="/2" symbol="05"/>
<gate name="/3" symbol="05"/>
<gate name="/4" symbol="05"/>
<gate name="/5" symbol="05"/>
<gate name="/6" symbol="05"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="Y" pad="2"/>
<connect gate="/2" pin="A" pad="3"/>
<connect gate="/2" pin="Y" pad="4"/>
<connect gate="/3" pin="A" pad="5"/>
<connect gate="/3" pin="Y" pad="6"/>
<connect gate="/4" pin="A" pad="9"/>
<connect gate="/4" pin="Y" pad="8"/>
<connect gate="/5" pin="A" pad="11"/>
<connect gate="/5" pin="Y" pad="10"/>
<connect gate="/6" pin="A" pad="13"/>
<connect gate="/6" pin="Y" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*09" prefix="V">
<description>Quad 2-input &lt;b&gt;AND&lt;/b&gt; gate, open collector</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="09"/>
<gate name="/2" symbol="09"/>
<gate name="/3" symbol="09"/>
<gate name="/4" symbol="09"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*11" prefix="V">
<description>Triple 3-input &lt;b&gt;AND&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="11"/>
<gate name="/2" symbol="11"/>
<gate name="/3" symbol="11"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="C" pad="13"/>
<connect gate="/1" pin="Y" pad="12"/>
<connect gate="/2" pin="A" pad="3"/>
<connect gate="/2" pin="B" pad="4"/>
<connect gate="/2" pin="C" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="C" pad="11"/>
<connect gate="/3" pin="Y" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*14" prefix="V">
<description>Hex schmitt trigger &lt;b&gt;INVERTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="14"/>
<gate name="/2" symbol="14"/>
<gate name="/3" symbol="14"/>
<gate name="/4" symbol="14"/>
<gate name="/5" symbol="14"/>
<gate name="/6" symbol="14"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="Y" pad="2"/>
<connect gate="/2" pin="A" pad="3"/>
<connect gate="/2" pin="Y" pad="4"/>
<connect gate="/3" pin="A" pad="5"/>
<connect gate="/3" pin="Y" pad="6"/>
<connect gate="/4" pin="A" pad="9"/>
<connect gate="/4" pin="Y" pad="8"/>
<connect gate="/5" pin="A" pad="11"/>
<connect gate="/5" pin="Y" pad="10"/>
<connect gate="/6" pin="A" pad="13"/>
<connect gate="/6" pin="Y" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*20" prefix="V">
<description>Dual 4-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="20"/>
<gate name="/2" symbol="20"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="C" pad="4"/>
<connect gate="/1" pin="D" pad="5"/>
<connect gate="/1" pin="Y" pad="6"/>
<connect gate="/2" pin="A" pad="9"/>
<connect gate="/2" pin="B" pad="10"/>
<connect gate="/2" pin="C" pad="12"/>
<connect gate="/2" pin="D" pad="13"/>
<connect gate="/2" pin="Y" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*21" prefix="V">
<description>Dual 4-input &lt;b&gt;AND&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="21"/>
<gate name="/2" symbol="21"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="C" pad="4"/>
<connect gate="/1" pin="D" pad="5"/>
<connect gate="/1" pin="Y" pad="6"/>
<connect gate="/2" pin="A" pad="9"/>
<connect gate="/2" pin="B" pad="10"/>
<connect gate="/2" pin="C" pad="12"/>
<connect gate="/2" pin="D" pad="13"/>
<connect gate="/2" pin="Y" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*27" prefix="V">
<description>Triple 3-input &lt;b&gt;NOR&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="27"/>
<gate name="/2" symbol="27"/>
<gate name="/3" symbol="27"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="C" pad="13"/>
<connect gate="/1" pin="Y" pad="12"/>
<connect gate="/2" pin="A" pad="3"/>
<connect gate="/2" pin="B" pad="4"/>
<connect gate="/2" pin="C" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="C" pad="11"/>
<connect gate="/3" pin="Y" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*30" prefix="V">
<description>8-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="30"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="B" pad="2"/>
<connect gate="1" pin="C" pad="3"/>
<connect gate="1" pin="D" pad="4"/>
<connect gate="1" pin="E" pad="5"/>
<connect gate="1" pin="F" pad="6"/>
<connect gate="1" pin="G" pad="11"/>
<connect gate="1" pin="H" pad="12"/>
<connect gate="1" pin="Y" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*32" prefix="V">
<description>Quad 2-input &lt;b&gt;OR&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="32"/>
<gate name="/2" symbol="32"/>
<gate name="/3" symbol="32"/>
<gate name="/4" symbol="32"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*36" prefix="V">
<description>Quad 2-input &lt;b&gt;NOR&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="36"/>
<gate name="/2" symbol="36"/>
<gate name="/3" symbol="36"/>
<gate name="/4" symbol="36"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*42" prefix="V">
<description>4-line to 10-line &lt;b&gt;DECODER&lt;/b&gt; (1-of-10)</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="42"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="A" pad="15"/>
<connect gate="1" pin="B" pad="14"/>
<connect gate="1" pin="C" pad="13"/>
<connect gate="1" pin="D" pad="12"/>
<connect gate="1" pin="Y0" pad="1"/>
<connect gate="1" pin="Y1" pad="2"/>
<connect gate="1" pin="Y2" pad="3"/>
<connect gate="1" pin="Y3" pad="4"/>
<connect gate="1" pin="Y4" pad="5"/>
<connect gate="1" pin="Y5" pad="6"/>
<connect gate="1" pin="Y6" pad="7"/>
<connect gate="1" pin="Y7" pad="9"/>
<connect gate="1" pin="Y8" pad="10"/>
<connect gate="1" pin="Y9" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*51" prefix="V">
<description>&lt;b&gt;AND-OR-INVERT&lt;/b&gt; gates&lt;/a&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="51_2"/>
<gate name="/2" symbol="51_1"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="2"/>
<connect gate="/1" pin="B" pad="3"/>
<connect gate="/1" pin="C" pad="4"/>
<connect gate="/1" pin="D" pad="5"/>
<connect gate="/1" pin="Y" pad="6"/>
<connect gate="/2" pin="A" pad="1"/>
<connect gate="/2" pin="B" pad="12"/>
<connect gate="/2" pin="C" pad="13"/>
<connect gate="/2" pin="D" pad="9"/>
<connect gate="/2" pin="E" pad="10"/>
<connect gate="/2" pin="F" pad="11"/>
<connect gate="/2" pin="Y" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*73" prefix="V">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="73"/>
<gate name="/2" symbol="73"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="4"/>
<connect gate="/-UB" pin="-UB" pad="11"/>
<connect gate="/1" pin="!CLR" pad="2"/>
<connect gate="/1" pin="!Q" pad="13"/>
<connect gate="/1" pin="CLK" pad="1"/>
<connect gate="/1" pin="J" pad="14"/>
<connect gate="/1" pin="K" pad="3"/>
<connect gate="/1" pin="Q" pad="12"/>
<connect gate="/2" pin="!CLR" pad="6"/>
<connect gate="/2" pin="!Q" pad="8"/>
<connect gate="/2" pin="CLK" pad="5"/>
<connect gate="/2" pin="J" pad="7"/>
<connect gate="/2" pin="K" pad="10"/>
<connect gate="/2" pin="Q" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*74" prefix="V">
<description>Dual D type positive edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="74"/>
<gate name="/2" symbol="74"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="!CLR" pad="1"/>
<connect gate="/1" pin="!PRE" pad="4"/>
<connect gate="/1" pin="!Q" pad="6"/>
<connect gate="/1" pin="CLK" pad="3"/>
<connect gate="/1" pin="D" pad="2"/>
<connect gate="/1" pin="Q" pad="5"/>
<connect gate="/2" pin="!CLR" pad="13"/>
<connect gate="/2" pin="!PRE" pad="10"/>
<connect gate="/2" pin="!Q" pad="8"/>
<connect gate="/2" pin="CLK" pad="11"/>
<connect gate="/2" pin="D" pad="12"/>
<connect gate="/2" pin="Q" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*75" prefix="V">
<description>4-bit bistable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="75"/>
<gate name="/2" symbol="75"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="5"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="/1" pin="!1Q" pad="11"/>
<connect gate="/1" pin="!2Q" pad="8"/>
<connect gate="/1" pin="1C,2C" pad="4"/>
<connect gate="/1" pin="1D" pad="6"/>
<connect gate="/1" pin="1Q" pad="10"/>
<connect gate="/1" pin="2D" pad="7"/>
<connect gate="/1" pin="2Q" pad="9"/>
<connect gate="/2" pin="!1Q" pad="1"/>
<connect gate="/2" pin="!2Q" pad="14"/>
<connect gate="/2" pin="1C,2C" pad="13"/>
<connect gate="/2" pin="1D" pad="2"/>
<connect gate="/2" pin="1Q" pad="16"/>
<connect gate="/2" pin="2D" pad="3"/>
<connect gate="/2" pin="2Q" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*76" prefix="V">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="76"/>
<gate name="/2" symbol="76"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="5"/>
<connect gate="/-UB" pin="-UB" pad="13"/>
<connect gate="/1" pin="!CLR" pad="3"/>
<connect gate="/1" pin="!PRE" pad="2"/>
<connect gate="/1" pin="!Q" pad="14"/>
<connect gate="/1" pin="CLK" pad="1"/>
<connect gate="/1" pin="J" pad="4"/>
<connect gate="/1" pin="K" pad="16"/>
<connect gate="/1" pin="Q" pad="15"/>
<connect gate="/2" pin="!CLR" pad="8"/>
<connect gate="/2" pin="!PRE" pad="7"/>
<connect gate="/2" pin="!Q" pad="10"/>
<connect gate="/2" pin="CLK" pad="6"/>
<connect gate="/2" pin="J" pad="9"/>
<connect gate="/2" pin="K" pad="12"/>
<connect gate="/2" pin="Q" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*77" prefix="V">
<description>4-bit D &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="77"/>
<gate name="/2" symbol="77"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="4"/>
<connect gate="/-UB" pin="-UB" pad="11"/>
<connect gate="/1" pin="1C,2C" pad="3"/>
<connect gate="/1" pin="1D" pad="5"/>
<connect gate="/1" pin="1Q" pad="9"/>
<connect gate="/1" pin="2D" pad="6"/>
<connect gate="/1" pin="2Q" pad="8"/>
<connect gate="/2" pin="1C,2C" pad="12"/>
<connect gate="/2" pin="1D" pad="1"/>
<connect gate="/2" pin="1Q" pad="14"/>
<connect gate="/2" pin="2D" pad="2"/>
<connect gate="/2" pin="2Q" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*78" prefix="V">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset, common clock and common clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="78"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="4"/>
<connect gate="/-UB" pin="-UB" pad="11"/>
<connect gate="1" pin="!1PRE" pad="2"/>
<connect gate="1" pin="!1Q" pad="12"/>
<connect gate="1" pin="!2PRE" pad="6"/>
<connect gate="1" pin="!2Q" pad="9"/>
<connect gate="1" pin="!CLR" pad="5"/>
<connect gate="1" pin="1J" pad="3"/>
<connect gate="1" pin="1K" pad="14"/>
<connect gate="1" pin="1Q" pad="13"/>
<connect gate="1" pin="2J" pad="10"/>
<connect gate="1" pin="2K" pad="7"/>
<connect gate="1" pin="2Q" pad="8"/>
<connect gate="1" pin="CLK" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*85A" prefix="V">
<description>4-bit Magnitude &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="85A"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="P0" pad="10"/>
<connect gate="1" pin="P1" pad="12"/>
<connect gate="1" pin="P2" pad="13"/>
<connect gate="1" pin="P3" pad="15"/>
<connect gate="1" pin="PEQQ" pad="6"/>
<connect gate="1" pin="PEQQ_" pad="3"/>
<connect gate="1" pin="PGTQ" pad="5"/>
<connect gate="1" pin="PGTQ_" pad="4"/>
<connect gate="1" pin="PLTQ" pad="7"/>
<connect gate="1" pin="PLTQ_" pad="2"/>
<connect gate="1" pin="Q0" pad="9"/>
<connect gate="1" pin="Q1" pad="11"/>
<connect gate="1" pin="Q2" pad="14"/>
<connect gate="1" pin="Q3" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*86" prefix="V">
<description>Quad 2-input &lt;b&gt;EXCLUSIV-OR&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="86"/>
<gate name="/2" symbol="86"/>
<gate name="/3" symbol="86"/>
<gate name="/4" symbol="86"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*107" prefix="V">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="107"/>
<gate name="/2" symbol="107"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="!CLR" pad="13"/>
<connect gate="/1" pin="!Q" pad="2"/>
<connect gate="/1" pin="CLK" pad="12"/>
<connect gate="/1" pin="J" pad="1"/>
<connect gate="/1" pin="K" pad="4"/>
<connect gate="/1" pin="Q" pad="3"/>
<connect gate="/2" pin="!CLR" pad="10"/>
<connect gate="/2" pin="!Q" pad="6"/>
<connect gate="/2" pin="CLK" pad="9"/>
<connect gate="/2" pin="J" pad="8"/>
<connect gate="/2" pin="K" pad="11"/>
<connect gate="/2" pin="Q" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*109" prefix="V">
<description>Dual J-K positive edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="109"/>
<gate name="/2" symbol="109"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="!CLR" pad="1"/>
<connect gate="/1" pin="!K" pad="3"/>
<connect gate="/1" pin="!PRE" pad="5"/>
<connect gate="/1" pin="!Q" pad="7"/>
<connect gate="/1" pin="CLK" pad="4"/>
<connect gate="/1" pin="J" pad="2"/>
<connect gate="/1" pin="Q" pad="6"/>
<connect gate="/2" pin="!CLR" pad="15"/>
<connect gate="/2" pin="!K" pad="13"/>
<connect gate="/2" pin="!PRE" pad="11"/>
<connect gate="/2" pin="!Q" pad="9"/>
<connect gate="/2" pin="CLK" pad="12"/>
<connect gate="/2" pin="J" pad="14"/>
<connect gate="/2" pin="Q" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*112" prefix="V">
<description>Dual J-K negative edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset and clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="112"/>
<gate name="/2" symbol="112"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="!CLR" pad="15"/>
<connect gate="/1" pin="!PRE" pad="4"/>
<connect gate="/1" pin="!Q" pad="6"/>
<connect gate="/1" pin="CLK" pad="1"/>
<connect gate="/1" pin="J" pad="3"/>
<connect gate="/1" pin="K" pad="2"/>
<connect gate="/1" pin="Q" pad="5"/>
<connect gate="/2" pin="!CLR" pad="14"/>
<connect gate="/2" pin="!PRE" pad="10"/>
<connect gate="/2" pin="!Q" pad="7"/>
<connect gate="/2" pin="CLK" pad="13"/>
<connect gate="/2" pin="J" pad="11"/>
<connect gate="/2" pin="K" pad="12"/>
<connect gate="/2" pin="Q" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*113" prefix="V">
<description>Dual J-K negative edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="113"/>
<gate name="/2" symbol="113"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="!PRE" pad="4"/>
<connect gate="/1" pin="!Q" pad="6"/>
<connect gate="/1" pin="CLK" pad="1"/>
<connect gate="/1" pin="J" pad="3"/>
<connect gate="/1" pin="K" pad="2"/>
<connect gate="/1" pin="Q" pad="5"/>
<connect gate="/2" pin="!PRE" pad="10"/>
<connect gate="/2" pin="!Q" pad="8"/>
<connect gate="/2" pin="CLK" pad="13"/>
<connect gate="/2" pin="J" pad="11"/>
<connect gate="/2" pin="K" pad="12"/>
<connect gate="/2" pin="Q" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*114" prefix="V">
<description>Dual J-K negative edge triggered &lt;b&gt;FLIP FLOP&lt;/b&gt;, preset, common clear, clock</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="114"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="!1PRE" pad="4"/>
<connect gate="1" pin="!1Q" pad="6"/>
<connect gate="1" pin="!2PRE" pad="10"/>
<connect gate="1" pin="!2Q" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="1J" pad="3"/>
<connect gate="1" pin="1K" pad="2"/>
<connect gate="1" pin="1Q" pad="5"/>
<connect gate="1" pin="2J" pad="11"/>
<connect gate="1" pin="2K" pad="12"/>
<connect gate="1" pin="2Q" pad="9"/>
<connect gate="1" pin="CLK" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*125" prefix="V">
<description>Quad bus &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="125"/>
<gate name="/2" symbol="125"/>
<gate name="/3" symbol="125"/>
<gate name="/4" symbol="125"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="!G" pad="1"/>
<connect gate="/1" pin="A" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="!G" pad="4"/>
<connect gate="/2" pin="A" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="!G" pad="10"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="!G" pad="13"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*126" prefix="V">
<description>Quad bus &lt;b&gt;BUFFER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="126"/>
<gate name="/2" symbol="126"/>
<gate name="/3" symbol="126"/>
<gate name="/4" symbol="126"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="2"/>
<connect gate="/1" pin="G" pad="1"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="5"/>
<connect gate="/2" pin="G" pad="4"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="G" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="G" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*132" prefix="V">
<description>Quad 2-input &lt;b&gt;NAND&lt;/b&gt; schmitt trigger</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="132"/>
<gate name="/2" symbol="132"/>
<gate name="/3" symbol="132"/>
<gate name="/4" symbol="132"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*133" prefix="V">
<description>13-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="133"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="B" pad="2"/>
<connect gate="1" pin="C" pad="3"/>
<connect gate="1" pin="D" pad="4"/>
<connect gate="1" pin="E" pad="5"/>
<connect gate="1" pin="F" pad="6"/>
<connect gate="1" pin="G" pad="7"/>
<connect gate="1" pin="H" pad="10"/>
<connect gate="1" pin="I" pad="11"/>
<connect gate="1" pin="J" pad="12"/>
<connect gate="1" pin="K" pad="13"/>
<connect gate="1" pin="L" pad="14"/>
<connect gate="1" pin="M" pad="15"/>
<connect gate="1" pin="Y" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*137" prefix="V">
<description>3-line to 8-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;, address LATCH</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="137"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G2" pad="5"/>
<connect gate="1" pin="!GL" pad="4"/>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="B" pad="2"/>
<connect gate="1" pin="C" pad="3"/>
<connect gate="1" pin="G1" pad="6"/>
<connect gate="1" pin="Y0" pad="15"/>
<connect gate="1" pin="Y1" pad="14"/>
<connect gate="1" pin="Y2" pad="13"/>
<connect gate="1" pin="Y3" pad="12"/>
<connect gate="1" pin="Y4" pad="11"/>
<connect gate="1" pin="Y5" pad="10"/>
<connect gate="1" pin="Y6" pad="9"/>
<connect gate="1" pin="Y7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*138" prefix="V">
<description>3-line to 8-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="138"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G2A" pad="4"/>
<connect gate="1" pin="!G2B" pad="5"/>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="B" pad="2"/>
<connect gate="1" pin="C" pad="3"/>
<connect gate="1" pin="G1" pad="6"/>
<connect gate="1" pin="Y0" pad="15"/>
<connect gate="1" pin="Y1" pad="14"/>
<connect gate="1" pin="Y2" pad="13"/>
<connect gate="1" pin="Y3" pad="12"/>
<connect gate="1" pin="Y4" pad="11"/>
<connect gate="1" pin="Y5" pad="10"/>
<connect gate="1" pin="Y6" pad="9"/>
<connect gate="1" pin="Y7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*139" prefix="V">
<description>Dual 2-line to 4-line &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="139"/>
<gate name="/2" symbol="139"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="!G" pad="1"/>
<connect gate="/1" pin="A" pad="2"/>
<connect gate="/1" pin="B" pad="3"/>
<connect gate="/1" pin="Y0" pad="4"/>
<connect gate="/1" pin="Y1" pad="5"/>
<connect gate="/1" pin="Y2" pad="6"/>
<connect gate="/1" pin="Y3" pad="7"/>
<connect gate="/2" pin="!G" pad="15"/>
<connect gate="/2" pin="A" pad="14"/>
<connect gate="/2" pin="B" pad="13"/>
<connect gate="/2" pin="Y0" pad="12"/>
<connect gate="/2" pin="Y1" pad="11"/>
<connect gate="/2" pin="Y2" pad="10"/>
<connect gate="/2" pin="Y3" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*147" prefix="V">
<description>10-line to 4-line and 8-line to 3-line &lt;b&gt;PRIORITY DECODER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="147"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="1" pad="11"/>
<connect gate="1" pin="2" pad="12"/>
<connect gate="1" pin="3" pad="13"/>
<connect gate="1" pin="4" pad="1"/>
<connect gate="1" pin="5" pad="2"/>
<connect gate="1" pin="6" pad="3"/>
<connect gate="1" pin="7" pad="4"/>
<connect gate="1" pin="8" pad="5"/>
<connect gate="1" pin="9" pad="10"/>
<connect gate="1" pin="A" pad="9"/>
<connect gate="1" pin="B" pad="7"/>
<connect gate="1" pin="C" pad="6"/>
<connect gate="1" pin="D" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*148" prefix="V">
<description>10-line to 4-line and 8-line to 3-line &lt;b&gt;PRIORITY ENCODER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="148"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="0" pad="10"/>
<connect gate="1" pin="1" pad="11"/>
<connect gate="1" pin="2" pad="12"/>
<connect gate="1" pin="3" pad="13"/>
<connect gate="1" pin="4" pad="1"/>
<connect gate="1" pin="5" pad="2"/>
<connect gate="1" pin="6" pad="3"/>
<connect gate="1" pin="7" pad="4"/>
<connect gate="1" pin="A0" pad="9"/>
<connect gate="1" pin="A1" pad="7"/>
<connect gate="1" pin="A2" pad="6"/>
<connect gate="1" pin="EI" pad="5"/>
<connect gate="1" pin="EO" pad="15"/>
<connect gate="1" pin="GS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*151" prefix="V">
<description>Data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="151"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G" pad="7"/>
<connect gate="1" pin="A" pad="11"/>
<connect gate="1" pin="B" pad="10"/>
<connect gate="1" pin="C" pad="9"/>
<connect gate="1" pin="D0" pad="4"/>
<connect gate="1" pin="D1" pad="3"/>
<connect gate="1" pin="D2" pad="2"/>
<connect gate="1" pin="D3" pad="1"/>
<connect gate="1" pin="D4" pad="15"/>
<connect gate="1" pin="D5" pad="14"/>
<connect gate="1" pin="D6" pad="13"/>
<connect gate="1" pin="D7" pad="12"/>
<connect gate="1" pin="W" pad="6"/>
<connect gate="1" pin="Y" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*152" prefix="V">
<description>Data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="152"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="A" pad="10"/>
<connect gate="1" pin="B" pad="9"/>
<connect gate="1" pin="C" pad="8"/>
<connect gate="1" pin="D0" pad="5"/>
<connect gate="1" pin="D1" pad="4"/>
<connect gate="1" pin="D2" pad="3"/>
<connect gate="1" pin="D3" pad="2"/>
<connect gate="1" pin="D4" pad="1"/>
<connect gate="1" pin="D5" pad="13"/>
<connect gate="1" pin="D6" pad="12"/>
<connect gate="1" pin="D7" pad="11"/>
<connect gate="1" pin="W" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*153" prefix="V">
<description>Dual 4-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="153"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!1G" pad="1"/>
<connect gate="1" pin="!2G" pad="15"/>
<connect gate="1" pin="1C0" pad="6"/>
<connect gate="1" pin="1C1" pad="5"/>
<connect gate="1" pin="1C2" pad="4"/>
<connect gate="1" pin="1C3" pad="3"/>
<connect gate="1" pin="1Y" pad="7"/>
<connect gate="1" pin="2C0" pad="10"/>
<connect gate="1" pin="2C1" pad="11"/>
<connect gate="1" pin="2C2" pad="12"/>
<connect gate="1" pin="2C3" pad="13"/>
<connect gate="1" pin="2Y" pad="9"/>
<connect gate="1" pin="A" pad="14"/>
<connect gate="1" pin="B" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*154" prefix="V">
<description>4-line to 16-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="154"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!G1" pad="18"/>
<connect gate="1" pin="!G2" pad="19"/>
<connect gate="1" pin="0" pad="1"/>
<connect gate="1" pin="1" pad="2"/>
<connect gate="1" pin="10" pad="11"/>
<connect gate="1" pin="11" pad="13"/>
<connect gate="1" pin="12" pad="14"/>
<connect gate="1" pin="13" pad="15"/>
<connect gate="1" pin="14" pad="16"/>
<connect gate="1" pin="15" pad="17"/>
<connect gate="1" pin="2" pad="3"/>
<connect gate="1" pin="3" pad="4"/>
<connect gate="1" pin="4" pad="5"/>
<connect gate="1" pin="5" pad="6"/>
<connect gate="1" pin="6" pad="7"/>
<connect gate="1" pin="7" pad="8"/>
<connect gate="1" pin="8" pad="9"/>
<connect gate="1" pin="9" pad="10"/>
<connect gate="1" pin="A" pad="23"/>
<connect gate="1" pin="B" pad="22"/>
<connect gate="1" pin="C" pad="21"/>
<connect gate="1" pin="D" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*157" prefix="V">
<description>Quadruple 2-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="157"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!A!/B" pad="1"/>
<connect gate="1" pin="!G" pad="15"/>
<connect gate="1" pin="1A" pad="2"/>
<connect gate="1" pin="1B" pad="3"/>
<connect gate="1" pin="1Y" pad="4"/>
<connect gate="1" pin="2A" pad="5"/>
<connect gate="1" pin="2B" pad="6"/>
<connect gate="1" pin="2Y" pad="7"/>
<connect gate="1" pin="3A" pad="11"/>
<connect gate="1" pin="3B" pad="10"/>
<connect gate="1" pin="3Y" pad="9"/>
<connect gate="1" pin="4A" pad="14"/>
<connect gate="1" pin="4B" pad="13"/>
<connect gate="1" pin="4Y" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*158" prefix="V">
<description>Quadruple 2-line to 1-line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="158"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!A!/B" pad="1"/>
<connect gate="1" pin="!G" pad="15"/>
<connect gate="1" pin="1A" pad="2"/>
<connect gate="1" pin="1B" pad="3"/>
<connect gate="1" pin="1Y" pad="4"/>
<connect gate="1" pin="2A" pad="5"/>
<connect gate="1" pin="2B" pad="6"/>
<connect gate="1" pin="2Y" pad="7"/>
<connect gate="1" pin="3A" pad="11"/>
<connect gate="1" pin="3B" pad="10"/>
<connect gate="1" pin="3Y" pad="9"/>
<connect gate="1" pin="4A" pad="14"/>
<connect gate="1" pin="4B" pad="13"/>
<connect gate="1" pin="4Y" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*160" prefix="V">
<description>Synchronous 4-bit &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="160"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="!LOAD" pad="9"/>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="B" pad="4"/>
<connect gate="1" pin="C" pad="5"/>
<connect gate="1" pin="CLK" pad="2"/>
<connect gate="1" pin="D" pad="6"/>
<connect gate="1" pin="ENP" pad="7"/>
<connect gate="1" pin="ENT" pad="10"/>
<connect gate="1" pin="QA" pad="14"/>
<connect gate="1" pin="QB" pad="13"/>
<connect gate="1" pin="QC" pad="12"/>
<connect gate="1" pin="QD" pad="11"/>
<connect gate="1" pin="RCO" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*162" prefix="V">
<description>Synchrounus 4-bit &lt;b&gt;COUNTER&lt;/b&gt; divide by 10</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="162"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="!LOAD" pad="9"/>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="B" pad="4"/>
<connect gate="1" pin="C" pad="5"/>
<connect gate="1" pin="CLK" pad="2"/>
<connect gate="1" pin="D" pad="6"/>
<connect gate="1" pin="ENP" pad="7"/>
<connect gate="1" pin="ENT" pad="10"/>
<connect gate="1" pin="QA" pad="14"/>
<connect gate="1" pin="QB" pad="13"/>
<connect gate="1" pin="QC" pad="12"/>
<connect gate="1" pin="QD" pad="11"/>
<connect gate="1" pin="RCO" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*161" prefix="V">
<description>Synchrounus 4-bit &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="161"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="!LOAD" pad="9"/>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="B" pad="4"/>
<connect gate="1" pin="C" pad="5"/>
<connect gate="1" pin="CLK" pad="2"/>
<connect gate="1" pin="D" pad="6"/>
<connect gate="1" pin="ENP" pad="7"/>
<connect gate="1" pin="ENT" pad="10"/>
<connect gate="1" pin="QA" pad="14"/>
<connect gate="1" pin="QB" pad="13"/>
<connect gate="1" pin="QC" pad="12"/>
<connect gate="1" pin="QD" pad="11"/>
<connect gate="1" pin="RCO" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*163" prefix="V">
<description>Synchrounus 4-bit &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="163"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="!LOAD" pad="9"/>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="B" pad="4"/>
<connect gate="1" pin="C" pad="5"/>
<connect gate="1" pin="CLK" pad="2"/>
<connect gate="1" pin="D" pad="6"/>
<connect gate="1" pin="ENP" pad="7"/>
<connect gate="1" pin="ENT" pad="10"/>
<connect gate="1" pin="QA" pad="14"/>
<connect gate="1" pin="QB" pad="13"/>
<connect gate="1" pin="QC" pad="12"/>
<connect gate="1" pin="QD" pad="11"/>
<connect gate="1" pin="RCO" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*164" prefix="V">
<description>8-bit parallel out &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="164"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="!CLR" pad="9"/>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="B" pad="2"/>
<connect gate="1" pin="CLK" pad="8"/>
<connect gate="1" pin="QA" pad="3"/>
<connect gate="1" pin="QB" pad="4"/>
<connect gate="1" pin="QC" pad="5"/>
<connect gate="1" pin="QD" pad="6"/>
<connect gate="1" pin="QE" pad="10"/>
<connect gate="1" pin="QF" pad="11"/>
<connect gate="1" pin="QG" pad="12"/>
<connect gate="1" pin="QH" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*165" prefix="V">
<description>8-bit parallel load &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="165"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!QH" pad="7"/>
<connect gate="1" pin="A" pad="11"/>
<connect gate="1" pin="B" pad="12"/>
<connect gate="1" pin="C" pad="13"/>
<connect gate="1" pin="CLK" pad="2"/>
<connect gate="1" pin="CLK_INH" pad="15"/>
<connect gate="1" pin="D" pad="14"/>
<connect gate="1" pin="E" pad="3"/>
<connect gate="1" pin="F" pad="4"/>
<connect gate="1" pin="G" pad="5"/>
<connect gate="1" pin="H" pad="6"/>
<connect gate="1" pin="QH" pad="9"/>
<connect gate="1" pin="SER" pad="10"/>
<connect gate="1" pin="SH/!LD" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*166" prefix="V">
<description>8-bit parallel load &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="166"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="9"/>
<connect gate="1" pin="A" pad="2"/>
<connect gate="1" pin="B" pad="3"/>
<connect gate="1" pin="C" pad="4"/>
<connect gate="1" pin="CLK" pad="7"/>
<connect gate="1" pin="CLK_INH" pad="6"/>
<connect gate="1" pin="D" pad="5"/>
<connect gate="1" pin="E" pad="10"/>
<connect gate="1" pin="F" pad="11"/>
<connect gate="1" pin="G" pad="12"/>
<connect gate="1" pin="H" pad="14"/>
<connect gate="1" pin="QH" pad="13"/>
<connect gate="1" pin="SER" pad="1"/>
<connect gate="1" pin="SH/!LD" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*173" prefix="V">
<description>4-bit D type &lt;b&gt;REGISTER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="173"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G1" pad="9"/>
<connect gate="1" pin="!G2" pad="10"/>
<connect gate="1" pin="1D" pad="14"/>
<connect gate="1" pin="1Q" pad="3"/>
<connect gate="1" pin="2D" pad="13"/>
<connect gate="1" pin="2Q" pad="4"/>
<connect gate="1" pin="3D" pad="12"/>
<connect gate="1" pin="3Q" pad="5"/>
<connect gate="1" pin="4D" pad="11"/>
<connect gate="1" pin="4Q" pad="6"/>
<connect gate="1" pin="CLK" pad="7"/>
<connect gate="1" pin="CLR" pad="15"/>
<connect gate="1" pin="M" pad="1"/>
<connect gate="1" pin="N" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*174" prefix="V">
<description>Hex D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="174"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="1D" pad="3"/>
<connect gate="1" pin="1Q" pad="2"/>
<connect gate="1" pin="2D" pad="4"/>
<connect gate="1" pin="2Q" pad="5"/>
<connect gate="1" pin="3D" pad="6"/>
<connect gate="1" pin="3Q" pad="7"/>
<connect gate="1" pin="4D" pad="11"/>
<connect gate="1" pin="4Q" pad="10"/>
<connect gate="1" pin="5D" pad="13"/>
<connect gate="1" pin="5Q" pad="12"/>
<connect gate="1" pin="6D" pad="14"/>
<connect gate="1" pin="6Q" pad="15"/>
<connect gate="1" pin="CLK" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*175" prefix="V">
<description>Qadruple D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="175"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!1Q" pad="3"/>
<connect gate="1" pin="!2Q" pad="6"/>
<connect gate="1" pin="!3Q" pad="11"/>
<connect gate="1" pin="!4Q" pad="14"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="1D" pad="4"/>
<connect gate="1" pin="1Q" pad="2"/>
<connect gate="1" pin="2D" pad="5"/>
<connect gate="1" pin="2Q" pad="7"/>
<connect gate="1" pin="3D" pad="12"/>
<connect gate="1" pin="3Q" pad="10"/>
<connect gate="1" pin="4D" pad="13"/>
<connect gate="1" pin="4Q" pad="15"/>
<connect gate="1" pin="CLK" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*180" prefix="V">
<description>9-bit odd/even &lt;B&gt;PARITY GENERATOR/CHECKER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="180"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="A" pad="8"/>
<connect gate="1" pin="B" pad="9"/>
<connect gate="1" pin="C" pad="10"/>
<connect gate="1" pin="D" pad="11"/>
<connect gate="1" pin="E" pad="12"/>
<connect gate="1" pin="EVEN" pad="3"/>
<connect gate="1" pin="F" pad="13"/>
<connect gate="1" pin="G" pad="1"/>
<connect gate="1" pin="H" pad="2"/>
<connect gate="1" pin="ODD" pad="4"/>
<connect gate="1" pin="SEVEN" pad="5"/>
<connect gate="1" pin="SODD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*190" prefix="V">
<description>Synchronous up down &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="190"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CTEN" pad="4"/>
<connect gate="1" pin="!LOAD" pad="11"/>
<connect gate="1" pin="!RCO" pad="13"/>
<connect gate="1" pin="A" pad="15"/>
<connect gate="1" pin="B" pad="1"/>
<connect gate="1" pin="C" pad="10"/>
<connect gate="1" pin="CLK" pad="14"/>
<connect gate="1" pin="D" pad="9"/>
<connect gate="1" pin="D/!U" pad="5"/>
<connect gate="1" pin="MAX/MIN" pad="12"/>
<connect gate="1" pin="QA" pad="3"/>
<connect gate="1" pin="QB" pad="2"/>
<connect gate="1" pin="QC" pad="6"/>
<connect gate="1" pin="QD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*191" prefix="V">
<description>Synchronous up down &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="191"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CTEN" pad="4"/>
<connect gate="1" pin="!LOAD" pad="11"/>
<connect gate="1" pin="!RCO" pad="13"/>
<connect gate="1" pin="A" pad="15"/>
<connect gate="1" pin="B" pad="1"/>
<connect gate="1" pin="C" pad="10"/>
<connect gate="1" pin="CLK" pad="14"/>
<connect gate="1" pin="D" pad="9"/>
<connect gate="1" pin="D/!U" pad="5"/>
<connect gate="1" pin="MAX/MIN" pad="12"/>
<connect gate="1" pin="QA" pad="3"/>
<connect gate="1" pin="QB" pad="2"/>
<connect gate="1" pin="QC" pad="6"/>
<connect gate="1" pin="QD" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*192" prefix="V">
<description>Synchronous 4-bit up down &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="192"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!BO" pad="13"/>
<connect gate="1" pin="!CO" pad="12"/>
<connect gate="1" pin="!LOAD" pad="11"/>
<connect gate="1" pin="A" pad="15"/>
<connect gate="1" pin="B" pad="1"/>
<connect gate="1" pin="C" pad="10"/>
<connect gate="1" pin="CLR" pad="14"/>
<connect gate="1" pin="D" pad="9"/>
<connect gate="1" pin="DOWN" pad="4"/>
<connect gate="1" pin="QA" pad="3"/>
<connect gate="1" pin="QB" pad="2"/>
<connect gate="1" pin="QC" pad="6"/>
<connect gate="1" pin="QD" pad="7"/>
<connect gate="1" pin="UP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*193" prefix="V">
<description>Synchronus 4-bit up down &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="193"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!BO" pad="13"/>
<connect gate="1" pin="!CO" pad="12"/>
<connect gate="1" pin="!LOAD" pad="11"/>
<connect gate="1" pin="A" pad="15"/>
<connect gate="1" pin="B" pad="1"/>
<connect gate="1" pin="C" pad="10"/>
<connect gate="1" pin="CLR" pad="14"/>
<connect gate="1" pin="D" pad="9"/>
<connect gate="1" pin="DOWN" pad="4"/>
<connect gate="1" pin="QA" pad="3"/>
<connect gate="1" pin="QB" pad="2"/>
<connect gate="1" pin="QC" pad="6"/>
<connect gate="1" pin="QD" pad="7"/>
<connect gate="1" pin="UP" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*194" prefix="V">
<description>4-bit bidirectional &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="194"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="B" pad="4"/>
<connect gate="1" pin="C" pad="5"/>
<connect gate="1" pin="CLK" pad="11"/>
<connect gate="1" pin="D" pad="6"/>
<connect gate="1" pin="QA" pad="15"/>
<connect gate="1" pin="QB" pad="14"/>
<connect gate="1" pin="QC" pad="13"/>
<connect gate="1" pin="QD" pad="12"/>
<connect gate="1" pin="S0" pad="9"/>
<connect gate="1" pin="S1" pad="10"/>
<connect gate="1" pin="SL_SER" pad="7"/>
<connect gate="1" pin="SR_SER" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*195" prefix="V">
<description>4-bit parallel access &lt;b&gt;SHIFT REGISTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="195"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="!K" pad="3"/>
<connect gate="1" pin="!QD" pad="11"/>
<connect gate="1" pin="A" pad="4"/>
<connect gate="1" pin="B" pad="5"/>
<connect gate="1" pin="C" pad="6"/>
<connect gate="1" pin="CLK" pad="10"/>
<connect gate="1" pin="D" pad="7"/>
<connect gate="1" pin="J" pad="2"/>
<connect gate="1" pin="QA" pad="15"/>
<connect gate="1" pin="QB" pad="14"/>
<connect gate="1" pin="QC" pad="13"/>
<connect gate="1" pin="QD" pad="12"/>
<connect gate="1" pin="SH/!LD" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*237" prefix="V">
<description>1 of 8 noninverting &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;, latches</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="237"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G2" pad="5"/>
<connect gate="1" pin="!GL" pad="4"/>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="B" pad="2"/>
<connect gate="1" pin="C" pad="3"/>
<connect gate="1" pin="G1" pad="6"/>
<connect gate="1" pin="Y0" pad="15"/>
<connect gate="1" pin="Y1" pad="14"/>
<connect gate="1" pin="Y2" pad="13"/>
<connect gate="1" pin="Y3" pad="12"/>
<connect gate="1" pin="Y4" pad="11"/>
<connect gate="1" pin="Y5" pad="10"/>
<connect gate="1" pin="Y6" pad="9"/>
<connect gate="1" pin="Y7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*238" prefix="V">
<description>1 of 8 noninverting &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="238"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G2A" pad="4"/>
<connect gate="1" pin="!G2B" pad="5"/>
<connect gate="1" pin="A" pad="1"/>
<connect gate="1" pin="B" pad="2"/>
<connect gate="1" pin="C" pad="3"/>
<connect gate="1" pin="G1" pad="6"/>
<connect gate="1" pin="Y0" pad="15"/>
<connect gate="1" pin="Y1" pad="14"/>
<connect gate="1" pin="Y2" pad="13"/>
<connect gate="1" pin="Y3" pad="12"/>
<connect gate="1" pin="Y4" pad="11"/>
<connect gate="1" pin="Y5" pad="10"/>
<connect gate="1" pin="Y6" pad="9"/>
<connect gate="1" pin="Y7" pad="7"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*239" prefix="V">
<description>Dual 1 of 4 noninverting &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="239"/>
<gate name="/2" symbol="239"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="!G" pad="1"/>
<connect gate="/1" pin="A" pad="2"/>
<connect gate="/1" pin="B" pad="3"/>
<connect gate="/1" pin="Y0" pad="4"/>
<connect gate="/1" pin="Y1" pad="5"/>
<connect gate="/1" pin="Y2" pad="6"/>
<connect gate="/1" pin="Y3" pad="7"/>
<connect gate="/2" pin="!G" pad="15"/>
<connect gate="/2" pin="A" pad="14"/>
<connect gate="/2" pin="B" pad="13"/>
<connect gate="/2" pin="Y0" pad="12"/>
<connect gate="/2" pin="Y1" pad="11"/>
<connect gate="/2" pin="Y2" pad="10"/>
<connect gate="/2" pin="Y3" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*240" prefix="V">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="240"/>
<gate name="/2" symbol="240"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="/1" pin="!G" pad="1"/>
<connect gate="/1" pin="A1" pad="2"/>
<connect gate="/1" pin="A2" pad="4"/>
<connect gate="/1" pin="A3" pad="6"/>
<connect gate="/1" pin="A4" pad="8"/>
<connect gate="/1" pin="Y1" pad="18"/>
<connect gate="/1" pin="Y2" pad="16"/>
<connect gate="/1" pin="Y3" pad="14"/>
<connect gate="/1" pin="Y4" pad="12"/>
<connect gate="/2" pin="!G" pad="19"/>
<connect gate="/2" pin="A1" pad="11"/>
<connect gate="/2" pin="A2" pad="13"/>
<connect gate="/2" pin="A3" pad="15"/>
<connect gate="/2" pin="A4" pad="17"/>
<connect gate="/2" pin="Y1" pad="9"/>
<connect gate="/2" pin="Y2" pad="7"/>
<connect gate="/2" pin="Y3" pad="5"/>
<connect gate="/2" pin="Y4" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*241" prefix="V">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="241_1"/>
<gate name="/2" symbol="241_2"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="/1" pin="!G" pad="1"/>
<connect gate="/1" pin="A1" pad="2"/>
<connect gate="/1" pin="A2" pad="4"/>
<connect gate="/1" pin="A3" pad="6"/>
<connect gate="/1" pin="A4" pad="8"/>
<connect gate="/1" pin="Y1" pad="18"/>
<connect gate="/1" pin="Y2" pad="16"/>
<connect gate="/1" pin="Y3" pad="14"/>
<connect gate="/1" pin="Y4" pad="12"/>
<connect gate="/2" pin="A1" pad="11"/>
<connect gate="/2" pin="A2" pad="13"/>
<connect gate="/2" pin="A3" pad="15"/>
<connect gate="/2" pin="A4" pad="17"/>
<connect gate="/2" pin="G" pad="19"/>
<connect gate="/2" pin="Y1" pad="9"/>
<connect gate="/2" pin="Y2" pad="7"/>
<connect gate="/2" pin="Y3" pad="5"/>
<connect gate="/2" pin="Y4" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*242" prefix="V">
<description>Quadruple &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="242"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="A1" pad="3"/>
<connect gate="1" pin="A2" pad="4"/>
<connect gate="1" pin="A3" pad="5"/>
<connect gate="1" pin="A4" pad="6"/>
<connect gate="1" pin="B1" pad="11"/>
<connect gate="1" pin="B2" pad="10"/>
<connect gate="1" pin="B3" pad="9"/>
<connect gate="1" pin="B4" pad="8"/>
<connect gate="1" pin="G1" pad="1"/>
<connect gate="1" pin="G2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*243" prefix="V">
<description>Quadruple &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="243"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="A1" pad="3"/>
<connect gate="1" pin="A2" pad="4"/>
<connect gate="1" pin="A3" pad="5"/>
<connect gate="1" pin="A4" pad="6"/>
<connect gate="1" pin="B1" pad="11"/>
<connect gate="1" pin="B2" pad="10"/>
<connect gate="1" pin="B3" pad="9"/>
<connect gate="1" pin="B4" pad="8"/>
<connect gate="1" pin="G1" pad="1"/>
<connect gate="1" pin="G2" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*244" prefix="V">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="244"/>
<gate name="/2" symbol="244"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="/1" pin="!G" pad="1"/>
<connect gate="/1" pin="A1" pad="2"/>
<connect gate="/1" pin="A2" pad="4"/>
<connect gate="/1" pin="A3" pad="6"/>
<connect gate="/1" pin="A4" pad="8"/>
<connect gate="/1" pin="Y1" pad="18"/>
<connect gate="/1" pin="Y2" pad="16"/>
<connect gate="/1" pin="Y3" pad="14"/>
<connect gate="/1" pin="Y4" pad="12"/>
<connect gate="/2" pin="!G" pad="19"/>
<connect gate="/2" pin="A1" pad="11"/>
<connect gate="/2" pin="A2" pad="13"/>
<connect gate="/2" pin="A3" pad="15"/>
<connect gate="/2" pin="A4" pad="17"/>
<connect gate="/2" pin="Y1" pad="9"/>
<connect gate="/2" pin="Y2" pad="7"/>
<connect gate="/2" pin="Y3" pad="5"/>
<connect gate="/2" pin="Y4" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*245" prefix="V">
<description>Octal &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="245"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G" pad="19"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="B1" pad="18"/>
<connect gate="1" pin="B2" pad="17"/>
<connect gate="1" pin="B3" pad="16"/>
<connect gate="1" pin="B4" pad="15"/>
<connect gate="1" pin="B5" pad="14"/>
<connect gate="1" pin="B6" pad="13"/>
<connect gate="1" pin="B7" pad="12"/>
<connect gate="1" pin="B8" pad="11"/>
<connect gate="1" pin="DIR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*251" prefix="V">
<description>1 of 8 data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="251"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G" pad="7"/>
<connect gate="1" pin="A" pad="11"/>
<connect gate="1" pin="B" pad="10"/>
<connect gate="1" pin="C" pad="9"/>
<connect gate="1" pin="D0" pad="4"/>
<connect gate="1" pin="D1" pad="3"/>
<connect gate="1" pin="D2" pad="2"/>
<connect gate="1" pin="D3" pad="1"/>
<connect gate="1" pin="D4" pad="15"/>
<connect gate="1" pin="D5" pad="14"/>
<connect gate="1" pin="D6" pad="13"/>
<connect gate="1" pin="D7" pad="12"/>
<connect gate="1" pin="W" pad="6"/>
<connect gate="1" pin="Y" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*253" prefix="V">
<description>Dual 4-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="253"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!1G" pad="1"/>
<connect gate="1" pin="!2G" pad="15"/>
<connect gate="1" pin="1C0" pad="6"/>
<connect gate="1" pin="1C1" pad="5"/>
<connect gate="1" pin="1C2" pad="4"/>
<connect gate="1" pin="1C3" pad="3"/>
<connect gate="1" pin="1Y" pad="7"/>
<connect gate="1" pin="2C0" pad="10"/>
<connect gate="1" pin="2C1" pad="11"/>
<connect gate="1" pin="2C2" pad="12"/>
<connect gate="1" pin="2C3" pad="13"/>
<connect gate="1" pin="2Y" pad="9"/>
<connect gate="1" pin="A" pad="14"/>
<connect gate="1" pin="B" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*257" prefix="V">
<description>Quadruple 2-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="257"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!A!/B" pad="1"/>
<connect gate="1" pin="!G" pad="15"/>
<connect gate="1" pin="1A" pad="2"/>
<connect gate="1" pin="1B" pad="3"/>
<connect gate="1" pin="1Y" pad="4"/>
<connect gate="1" pin="2A" pad="5"/>
<connect gate="1" pin="2B" pad="6"/>
<connect gate="1" pin="2Y" pad="7"/>
<connect gate="1" pin="3A" pad="11"/>
<connect gate="1" pin="3B" pad="10"/>
<connect gate="1" pin="3Y" pad="9"/>
<connect gate="1" pin="4A" pad="14"/>
<connect gate="1" pin="4B" pad="13"/>
<connect gate="1" pin="4Y" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*258" prefix="V">
<description>Quadruple 2-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="258"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G" pad="15"/>
<connect gate="1" pin="1A" pad="2"/>
<connect gate="1" pin="1B" pad="3"/>
<connect gate="1" pin="1Y" pad="4"/>
<connect gate="1" pin="2A" pad="5"/>
<connect gate="1" pin="2B" pad="6"/>
<connect gate="1" pin="2Y" pad="7"/>
<connect gate="1" pin="3A" pad="11"/>
<connect gate="1" pin="3B" pad="10"/>
<connect gate="1" pin="3Y" pad="9"/>
<connect gate="1" pin="4A" pad="14"/>
<connect gate="1" pin="4B" pad="13"/>
<connect gate="1" pin="4Y" pad="12"/>
<connect gate="1" pin="A/!B" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*259" prefix="V">
<description>8-bit addressable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="259"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLR" pad="15"/>
<connect gate="1" pin="!G" pad="14"/>
<connect gate="1" pin="D" pad="13"/>
<connect gate="1" pin="Q0" pad="4"/>
<connect gate="1" pin="Q1" pad="5"/>
<connect gate="1" pin="Q2" pad="6"/>
<connect gate="1" pin="Q3" pad="7"/>
<connect gate="1" pin="Q4" pad="9"/>
<connect gate="1" pin="Q5" pad="10"/>
<connect gate="1" pin="Q6" pad="11"/>
<connect gate="1" pin="Q7" pad="12"/>
<connect gate="1" pin="S0" pad="1"/>
<connect gate="1" pin="S1" pad="2"/>
<connect gate="1" pin="S2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*266" prefix="V">
<description>Quadruple &lt;b&gt;EXCLUSIVE-NOR&lt;/b&gt;, open-collector</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="266"/>
<gate name="/2" symbol="266"/>
<gate name="/3" symbol="266"/>
<gate name="/4" symbol="266"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="5"/>
<connect gate="/2" pin="B" pad="6"/>
<connect gate="/2" pin="Y" pad="4"/>
<connect gate="/3" pin="A" pad="8"/>
<connect gate="/3" pin="B" pad="9"/>
<connect gate="/3" pin="Y" pad="10"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*273" prefix="V">
<description>Octal D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, clear</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="273"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!CLR" pad="1"/>
<connect gate="1" pin="1D" pad="3"/>
<connect gate="1" pin="1Q" pad="2"/>
<connect gate="1" pin="2D" pad="4"/>
<connect gate="1" pin="2Q" pad="5"/>
<connect gate="1" pin="3D" pad="7"/>
<connect gate="1" pin="3Q" pad="6"/>
<connect gate="1" pin="4D" pad="8"/>
<connect gate="1" pin="4Q" pad="9"/>
<connect gate="1" pin="5D" pad="13"/>
<connect gate="1" pin="5Q" pad="12"/>
<connect gate="1" pin="6D" pad="14"/>
<connect gate="1" pin="6Q" pad="15"/>
<connect gate="1" pin="7D" pad="17"/>
<connect gate="1" pin="7Q" pad="16"/>
<connect gate="1" pin="8D" pad="18"/>
<connect gate="1" pin="8Q" pad="19"/>
<connect gate="1" pin="CLK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*280" prefix="V">
<description>9-bit odd/even &lt;b&gt;PARITY GENERATOR/CHECKER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="280"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="A" pad="8"/>
<connect gate="1" pin="B" pad="9"/>
<connect gate="1" pin="C" pad="10"/>
<connect gate="1" pin="D" pad="11"/>
<connect gate="1" pin="E" pad="12"/>
<connect gate="1" pin="F" pad="13"/>
<connect gate="1" pin="G" pad="1"/>
<connect gate="1" pin="H" pad="2"/>
<connect gate="1" pin="I" pad="4"/>
<connect gate="1" pin="SEVEN" pad="5"/>
<connect gate="1" pin="SODD" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*283" prefix="V">
<description>4-bit binary &lt;b&gt;FULL ADDER&lt;/b&gt;, fast carry</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="283"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="A1" pad="5"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="14"/>
<connect gate="1" pin="A4" pad="12"/>
<connect gate="1" pin="B1" pad="6"/>
<connect gate="1" pin="B2" pad="2"/>
<connect gate="1" pin="B3" pad="15"/>
<connect gate="1" pin="B4" pad="11"/>
<connect gate="1" pin="C0" pad="7"/>
<connect gate="1" pin="C4" pad="9"/>
<connect gate="1" pin="S1" pad="4"/>
<connect gate="1" pin="S2" pad="1"/>
<connect gate="1" pin="S3" pad="13"/>
<connect gate="1" pin="S4" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*298" prefix="V">
<description>Quadruple 2-input &lt;b&gt;MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="298"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="A1" pad="3"/>
<connect gate="1" pin="A2" pad="2"/>
<connect gate="1" pin="B1" pad="4"/>
<connect gate="1" pin="B2" pad="1"/>
<connect gate="1" pin="C1" pad="9"/>
<connect gate="1" pin="C2" pad="5"/>
<connect gate="1" pin="CLK" pad="11"/>
<connect gate="1" pin="D1" pad="7"/>
<connect gate="1" pin="D2" pad="6"/>
<connect gate="1" pin="QA" pad="15"/>
<connect gate="1" pin="QB" pad="14"/>
<connect gate="1" pin="QC" pad="13"/>
<connect gate="1" pin="QD" pad="12"/>
<connect gate="1" pin="WS" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*299" prefix="V">
<description>8-bit universal &lt;b&gt;SHIFT/STORAGE REGISTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="299"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!CLR" pad="9"/>
<connect gate="1" pin="!G1" pad="2"/>
<connect gate="1" pin="!G2" pad="3"/>
<connect gate="1" pin="A/QA" pad="7"/>
<connect gate="1" pin="B/QB" pad="13"/>
<connect gate="1" pin="C/QC" pad="6"/>
<connect gate="1" pin="CLK" pad="12"/>
<connect gate="1" pin="D/QD" pad="14"/>
<connect gate="1" pin="E/QE" pad="5"/>
<connect gate="1" pin="F/QF" pad="15"/>
<connect gate="1" pin="G/QG" pad="4"/>
<connect gate="1" pin="H/QH" pad="16"/>
<connect gate="1" pin="QA*" pad="8"/>
<connect gate="1" pin="QH*" pad="17"/>
<connect gate="1" pin="S0" pad="1"/>
<connect gate="1" pin="S1" pad="19"/>
<connect gate="1" pin="SL" pad="18"/>
<connect gate="1" pin="SR" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*352" prefix="V">
<description>Dual 4-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="352"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!1G" pad="1"/>
<connect gate="1" pin="!2G" pad="15"/>
<connect gate="1" pin="1C0" pad="6"/>
<connect gate="1" pin="1C1" pad="5"/>
<connect gate="1" pin="1C2" pad="4"/>
<connect gate="1" pin="1C3" pad="3"/>
<connect gate="1" pin="1Y" pad="7"/>
<connect gate="1" pin="2C0" pad="10"/>
<connect gate="1" pin="2C1" pad="11"/>
<connect gate="1" pin="2C2" pad="12"/>
<connect gate="1" pin="2C3" pad="13"/>
<connect gate="1" pin="2Y" pad="9"/>
<connect gate="1" pin="A" pad="14"/>
<connect gate="1" pin="B" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*353" prefix="V">
<description>Dual 4-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="353"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!1G" pad="1"/>
<connect gate="1" pin="!2G" pad="15"/>
<connect gate="1" pin="1C0" pad="6"/>
<connect gate="1" pin="1C1" pad="5"/>
<connect gate="1" pin="1C2" pad="4"/>
<connect gate="1" pin="1C3" pad="3"/>
<connect gate="1" pin="1Y" pad="7"/>
<connect gate="1" pin="2C0" pad="10"/>
<connect gate="1" pin="2C1" pad="11"/>
<connect gate="1" pin="2C2" pad="12"/>
<connect gate="1" pin="2C3" pad="13"/>
<connect gate="1" pin="2Y" pad="9"/>
<connect gate="1" pin="A" pad="14"/>
<connect gate="1" pin="B" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*354" prefix="V">
<description>8-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER/REGISTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="354"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!DC" pad="9"/>
<connect gate="1" pin="!G1" pad="15"/>
<connect gate="1" pin="!G2" pad="16"/>
<connect gate="1" pin="!SC" pad="11"/>
<connect gate="1" pin="D0" pad="8"/>
<connect gate="1" pin="D1" pad="7"/>
<connect gate="1" pin="D2" pad="6"/>
<connect gate="1" pin="D3" pad="5"/>
<connect gate="1" pin="D4" pad="4"/>
<connect gate="1" pin="D5" pad="3"/>
<connect gate="1" pin="D6" pad="2"/>
<connect gate="1" pin="D7" pad="1"/>
<connect gate="1" pin="G3" pad="17"/>
<connect gate="1" pin="S0" pad="14"/>
<connect gate="1" pin="S1" pad="13"/>
<connect gate="1" pin="S2" pad="12"/>
<connect gate="1" pin="W" pad="18"/>
<connect gate="1" pin="Y" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*356" prefix="V">
<description>8-to 1 line data &lt;b&gt;SELECTOR/MULTIPLEXER/REGISTER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="356"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G1" pad="15"/>
<connect gate="1" pin="!G2" pad="16"/>
<connect gate="1" pin="!SC" pad="11"/>
<connect gate="1" pin="CLK" pad="9"/>
<connect gate="1" pin="D0" pad="8"/>
<connect gate="1" pin="D1" pad="7"/>
<connect gate="1" pin="D2" pad="6"/>
<connect gate="1" pin="D3" pad="5"/>
<connect gate="1" pin="D4" pad="4"/>
<connect gate="1" pin="D5" pad="3"/>
<connect gate="1" pin="D6" pad="2"/>
<connect gate="1" pin="D7" pad="1"/>
<connect gate="1" pin="G3" pad="17"/>
<connect gate="1" pin="S0" pad="14"/>
<connect gate="1" pin="S1" pad="13"/>
<connect gate="1" pin="S2" pad="12"/>
<connect gate="1" pin="W" pad="18"/>
<connect gate="1" pin="Y" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*365" prefix="V">
<description>Hex &lt;b&gt;BUS DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="365"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G1" pad="1"/>
<connect gate="1" pin="!G2" pad="15"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="4"/>
<connect gate="1" pin="A3" pad="6"/>
<connect gate="1" pin="A4" pad="10"/>
<connect gate="1" pin="A5" pad="12"/>
<connect gate="1" pin="A6" pad="14"/>
<connect gate="1" pin="Y1" pad="3"/>
<connect gate="1" pin="Y2" pad="5"/>
<connect gate="1" pin="Y3" pad="7"/>
<connect gate="1" pin="Y4" pad="9"/>
<connect gate="1" pin="Y5" pad="11"/>
<connect gate="1" pin="Y6" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*366" prefix="V">
<description>Hex &lt;b&gt;BUS DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="366"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G1" pad="1"/>
<connect gate="1" pin="!G2" pad="15"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="4"/>
<connect gate="1" pin="A3" pad="6"/>
<connect gate="1" pin="A4" pad="10"/>
<connect gate="1" pin="A5" pad="12"/>
<connect gate="1" pin="A6" pad="14"/>
<connect gate="1" pin="Y1" pad="3"/>
<connect gate="1" pin="Y2" pad="5"/>
<connect gate="1" pin="Y3" pad="7"/>
<connect gate="1" pin="Y4" pad="9"/>
<connect gate="1" pin="Y5" pad="11"/>
<connect gate="1" pin="Y6" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*367" prefix="V">
<description>Hex &lt;b&gt;BUS DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="367_2"/>
<gate name="/2" symbol="367_1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="!G" pad="15"/>
<connect gate="/1" pin="A1" pad="12"/>
<connect gate="/1" pin="A2" pad="14"/>
<connect gate="/1" pin="Y1" pad="11"/>
<connect gate="/1" pin="Y2" pad="13"/>
<connect gate="/2" pin="!G" pad="1"/>
<connect gate="/2" pin="A1" pad="2"/>
<connect gate="/2" pin="A2" pad="4"/>
<connect gate="/2" pin="A3" pad="6"/>
<connect gate="/2" pin="A4" pad="10"/>
<connect gate="/2" pin="Y1" pad="3"/>
<connect gate="/2" pin="Y2" pad="5"/>
<connect gate="/2" pin="Y3" pad="7"/>
<connect gate="/2" pin="Y4" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*368" prefix="V">
<description>Hex &lt;b&gt;BUS DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="368_2"/>
<gate name="/2" symbol="368_1"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="!G" pad="15"/>
<connect gate="/1" pin="A1" pad="12"/>
<connect gate="/1" pin="A2" pad="14"/>
<connect gate="/1" pin="Y1" pad="11"/>
<connect gate="/1" pin="Y2" pad="13"/>
<connect gate="/2" pin="!G" pad="1"/>
<connect gate="/2" pin="A1" pad="2"/>
<connect gate="/2" pin="A2" pad="4"/>
<connect gate="/2" pin="A3" pad="6"/>
<connect gate="/2" pin="A4" pad="10"/>
<connect gate="/2" pin="Y1" pad="3"/>
<connect gate="/2" pin="Y2" pad="5"/>
<connect gate="/2" pin="Y3" pad="7"/>
<connect gate="/2" pin="Y4" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*373" prefix="V">
<description>Octal D type transparent &lt;b&gt;LATCH&lt;/b&gt;, edge triggered</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="373"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!OC" pad="1"/>
<connect gate="1" pin="1D" pad="3"/>
<connect gate="1" pin="1Q" pad="2"/>
<connect gate="1" pin="2D" pad="4"/>
<connect gate="1" pin="2Q" pad="5"/>
<connect gate="1" pin="3D" pad="7"/>
<connect gate="1" pin="3Q" pad="6"/>
<connect gate="1" pin="4D" pad="8"/>
<connect gate="1" pin="4Q" pad="9"/>
<connect gate="1" pin="5D" pad="13"/>
<connect gate="1" pin="5Q" pad="12"/>
<connect gate="1" pin="6D" pad="14"/>
<connect gate="1" pin="6Q" pad="15"/>
<connect gate="1" pin="7D" pad="17"/>
<connect gate="1" pin="7Q" pad="16"/>
<connect gate="1" pin="8D" pad="18"/>
<connect gate="1" pin="8Q" pad="19"/>
<connect gate="1" pin="C" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*374" prefix="V">
<description>Octal D type transparent &lt;b&gt;LATCH&lt;/b&gt;, edge triggered</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="374"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!OC" pad="1"/>
<connect gate="1" pin="1D" pad="3"/>
<connect gate="1" pin="1Q" pad="2"/>
<connect gate="1" pin="2D" pad="4"/>
<connect gate="1" pin="2Q" pad="5"/>
<connect gate="1" pin="3D" pad="7"/>
<connect gate="1" pin="3Q" pad="6"/>
<connect gate="1" pin="4D" pad="8"/>
<connect gate="1" pin="4Q" pad="9"/>
<connect gate="1" pin="5D" pad="13"/>
<connect gate="1" pin="5Q" pad="12"/>
<connect gate="1" pin="6D" pad="14"/>
<connect gate="1" pin="6Q" pad="15"/>
<connect gate="1" pin="7D" pad="17"/>
<connect gate="1" pin="7Q" pad="16"/>
<connect gate="1" pin="8D" pad="18"/>
<connect gate="1" pin="8Q" pad="19"/>
<connect gate="1" pin="CLK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*375" prefix="V">
<description>4-bit bistable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="375"/>
<gate name="/2" symbol="375"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="!1Q" pad="2"/>
<connect gate="/1" pin="!2Q" pad="6"/>
<connect gate="/1" pin="1C,2C" pad="4"/>
<connect gate="/1" pin="1D" pad="1"/>
<connect gate="/1" pin="1Q" pad="3"/>
<connect gate="/1" pin="2D" pad="7"/>
<connect gate="/1" pin="2Q" pad="5"/>
<connect gate="/2" pin="!1Q" pad="10"/>
<connect gate="/2" pin="!2Q" pad="14"/>
<connect gate="/2" pin="1C,2C" pad="12"/>
<connect gate="/2" pin="1D" pad="9"/>
<connect gate="/2" pin="1Q" pad="11"/>
<connect gate="/2" pin="2D" pad="15"/>
<connect gate="/2" pin="2Q" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*377" prefix="V">
<description>Octal D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, enable</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="377"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G" pad="1"/>
<connect gate="1" pin="1D" pad="3"/>
<connect gate="1" pin="1Q" pad="2"/>
<connect gate="1" pin="2D" pad="4"/>
<connect gate="1" pin="2Q" pad="5"/>
<connect gate="1" pin="3D" pad="7"/>
<connect gate="1" pin="3Q" pad="6"/>
<connect gate="1" pin="4D" pad="8"/>
<connect gate="1" pin="4Q" pad="9"/>
<connect gate="1" pin="5D" pad="13"/>
<connect gate="1" pin="5Q" pad="12"/>
<connect gate="1" pin="6D" pad="14"/>
<connect gate="1" pin="6Q" pad="15"/>
<connect gate="1" pin="7D" pad="17"/>
<connect gate="1" pin="7Q" pad="16"/>
<connect gate="1" pin="8D" pad="18"/>
<connect gate="1" pin="8Q" pad="19"/>
<connect gate="1" pin="CLK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*378" prefix="V">
<description>Hex D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, enable</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="378"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G" pad="1"/>
<connect gate="1" pin="1D" pad="3"/>
<connect gate="1" pin="1Q" pad="2"/>
<connect gate="1" pin="2D" pad="4"/>
<connect gate="1" pin="2Q" pad="5"/>
<connect gate="1" pin="3D" pad="6"/>
<connect gate="1" pin="3Q" pad="7"/>
<connect gate="1" pin="4D" pad="11"/>
<connect gate="1" pin="4Q" pad="10"/>
<connect gate="1" pin="5D" pad="13"/>
<connect gate="1" pin="5Q" pad="12"/>
<connect gate="1" pin="6D" pad="14"/>
<connect gate="1" pin="6Q" pad="15"/>
<connect gate="1" pin="CLK" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*379" prefix="V">
<description>Quad D type &lt;b&gt;FLIP FLOP&lt;/b&gt;, enable</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="379"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!1Q" pad="3"/>
<connect gate="1" pin="!2Q" pad="6"/>
<connect gate="1" pin="!3Q" pad="11"/>
<connect gate="1" pin="!4Q" pad="14"/>
<connect gate="1" pin="!G" pad="1"/>
<connect gate="1" pin="1D" pad="4"/>
<connect gate="1" pin="1Q" pad="2"/>
<connect gate="1" pin="2D" pad="5"/>
<connect gate="1" pin="2Q" pad="7"/>
<connect gate="1" pin="3D" pad="12"/>
<connect gate="1" pin="3Q" pad="10"/>
<connect gate="1" pin="4D" pad="13"/>
<connect gate="1" pin="4Q" pad="15"/>
<connect gate="1" pin="CLK" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*386" prefix="V">
<description>Quadruple 2-input &lt;b&gt;EXCLUSIVE-OR&lt;/b&gt; gate</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="386"/>
<gate name="/2" symbol="386"/>
<gate name="/3" symbol="386"/>
<gate name="/4" symbol="386"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="5"/>
<connect gate="/2" pin="B" pad="6"/>
<connect gate="/2" pin="Y" pad="4"/>
<connect gate="/3" pin="A" pad="8"/>
<connect gate="/3" pin="B" pad="9"/>
<connect gate="/3" pin="Y" pad="10"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*390" prefix="V">
<description>Dual 4-bit decade and binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="390"/>
<gate name="/2" symbol="390"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="CKA" pad="1"/>
<connect gate="/1" pin="CKB" pad="4"/>
<connect gate="/1" pin="CLR" pad="2"/>
<connect gate="/1" pin="QA" pad="3"/>
<connect gate="/1" pin="QB" pad="5"/>
<connect gate="/1" pin="QC" pad="6"/>
<connect gate="/1" pin="QD" pad="7"/>
<connect gate="/2" pin="CKA" pad="15"/>
<connect gate="/2" pin="CKB" pad="12"/>
<connect gate="/2" pin="CLR" pad="14"/>
<connect gate="/2" pin="QA" pad="13"/>
<connect gate="/2" pin="QB" pad="11"/>
<connect gate="/2" pin="QC" pad="10"/>
<connect gate="/2" pin="QD" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*393" prefix="V">
<description>Dual 4-bit decade and binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="393"/>
<gate name="/2" symbol="393"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="CLR" pad="2"/>
<connect gate="/1" pin="QA" pad="3"/>
<connect gate="/1" pin="QB" pad="4"/>
<connect gate="/1" pin="QC" pad="5"/>
<connect gate="/1" pin="QD" pad="6"/>
<connect gate="/2" pin="A" pad="13"/>
<connect gate="/2" pin="CLR" pad="12"/>
<connect gate="/2" pin="QA" pad="11"/>
<connect gate="/2" pin="QB" pad="10"/>
<connect gate="/2" pin="QC" pad="9"/>
<connect gate="/2" pin="QD" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*490" prefix="V">
<description>Dual 4-bit decade &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="490"/>
<gate name="/2" symbol="490"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="/1" pin="CLK" pad="1"/>
<connect gate="/1" pin="CLR" pad="2"/>
<connect gate="/1" pin="QA" pad="3"/>
<connect gate="/1" pin="QB" pad="5"/>
<connect gate="/1" pin="QC" pad="6"/>
<connect gate="/1" pin="QD" pad="7"/>
<connect gate="/1" pin="SET9" pad="4"/>
<connect gate="/2" pin="CLK" pad="15"/>
<connect gate="/2" pin="CLR" pad="14"/>
<connect gate="/2" pin="QA" pad="13"/>
<connect gate="/2" pin="QB" pad="11"/>
<connect gate="/2" pin="QC" pad="10"/>
<connect gate="/2" pin="QD" pad="9"/>
<connect gate="/2" pin="SET9" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*533" prefix="V">
<description>Inverting 8-bit D type &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="533"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!1Q" pad="2"/>
<connect gate="1" pin="!2Q" pad="5"/>
<connect gate="1" pin="!3Q" pad="6"/>
<connect gate="1" pin="!4Q" pad="9"/>
<connect gate="1" pin="!5Q" pad="12"/>
<connect gate="1" pin="!6Q" pad="15"/>
<connect gate="1" pin="!7Q" pad="16"/>
<connect gate="1" pin="!8Q" pad="19"/>
<connect gate="1" pin="!OC" pad="1"/>
<connect gate="1" pin="1D" pad="3"/>
<connect gate="1" pin="2D" pad="4"/>
<connect gate="1" pin="3D" pad="7"/>
<connect gate="1" pin="4D" pad="8"/>
<connect gate="1" pin="5D" pad="13"/>
<connect gate="1" pin="6D" pad="14"/>
<connect gate="1" pin="7D" pad="17"/>
<connect gate="1" pin="8D" pad="18"/>
<connect gate="1" pin="C" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*534" prefix="V">
<description>8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="534"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!1Q" pad="2"/>
<connect gate="1" pin="!2Q" pad="5"/>
<connect gate="1" pin="!3Q" pad="6"/>
<connect gate="1" pin="!4Q" pad="9"/>
<connect gate="1" pin="!5Q" pad="12"/>
<connect gate="1" pin="!6Q" pad="15"/>
<connect gate="1" pin="!7Q" pad="16"/>
<connect gate="1" pin="!8Q" pad="19"/>
<connect gate="1" pin="!OC" pad="1"/>
<connect gate="1" pin="1D" pad="3"/>
<connect gate="1" pin="2D" pad="4"/>
<connect gate="1" pin="3D" pad="7"/>
<connect gate="1" pin="4D" pad="8"/>
<connect gate="1" pin="5D" pad="13"/>
<connect gate="1" pin="6D" pad="14"/>
<connect gate="1" pin="7D" pad="17"/>
<connect gate="1" pin="8D" pad="18"/>
<connect gate="1" pin="CLK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*540" prefix="V">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="540"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G1" pad="1"/>
<connect gate="1" pin="!G2" pad="19"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="Y1" pad="18"/>
<connect gate="1" pin="Y2" pad="17"/>
<connect gate="1" pin="Y3" pad="16"/>
<connect gate="1" pin="Y4" pad="15"/>
<connect gate="1" pin="Y5" pad="14"/>
<connect gate="1" pin="Y6" pad="13"/>
<connect gate="1" pin="Y7" pad="12"/>
<connect gate="1" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*541" prefix="V">
<description>Octal &lt;b&gt;BUFFER&lt;/b&gt; and &lt;b&gt;LINE DRIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="541"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G1" pad="1"/>
<connect gate="1" pin="!G2" pad="19"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="Y1" pad="18"/>
<connect gate="1" pin="Y2" pad="17"/>
<connect gate="1" pin="Y3" pad="16"/>
<connect gate="1" pin="Y4" pad="15"/>
<connect gate="1" pin="Y5" pad="14"/>
<connect gate="1" pin="Y6" pad="13"/>
<connect gate="1" pin="Y7" pad="12"/>
<connect gate="1" pin="Y8" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*563" prefix="V">
<description>Inverting 8-bit D type &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="563"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!1Q" pad="19"/>
<connect gate="1" pin="!2Q" pad="18"/>
<connect gate="1" pin="!3Q" pad="17"/>
<connect gate="1" pin="!4Q" pad="16"/>
<connect gate="1" pin="!5Q" pad="15"/>
<connect gate="1" pin="!6Q" pad="14"/>
<connect gate="1" pin="!7Q" pad="13"/>
<connect gate="1" pin="!8Q" pad="12"/>
<connect gate="1" pin="!OC" pad="1"/>
<connect gate="1" pin="1D" pad="2"/>
<connect gate="1" pin="2D" pad="3"/>
<connect gate="1" pin="3D" pad="4"/>
<connect gate="1" pin="4D" pad="5"/>
<connect gate="1" pin="5D" pad="6"/>
<connect gate="1" pin="6D" pad="7"/>
<connect gate="1" pin="7D" pad="8"/>
<connect gate="1" pin="8D" pad="9"/>
<connect gate="1" pin="C" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*564" prefix="V">
<description>Inverting 8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="564"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!1Q" pad="19"/>
<connect gate="1" pin="!2Q" pad="18"/>
<connect gate="1" pin="!3Q" pad="17"/>
<connect gate="1" pin="!4Q" pad="16"/>
<connect gate="1" pin="!5Q" pad="15"/>
<connect gate="1" pin="!6Q" pad="14"/>
<connect gate="1" pin="!7Q" pad="13"/>
<connect gate="1" pin="!8Q" pad="12"/>
<connect gate="1" pin="!OC" pad="1"/>
<connect gate="1" pin="1D" pad="2"/>
<connect gate="1" pin="2D" pad="3"/>
<connect gate="1" pin="3D" pad="4"/>
<connect gate="1" pin="4D" pad="5"/>
<connect gate="1" pin="5D" pad="6"/>
<connect gate="1" pin="6D" pad="7"/>
<connect gate="1" pin="7D" pad="8"/>
<connect gate="1" pin="8D" pad="9"/>
<connect gate="1" pin="CLK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*573" prefix="V">
<description>8-bit D latch &lt;b&gt;BUS DRIVER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="573"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!OC" pad="1"/>
<connect gate="1" pin="1D" pad="2"/>
<connect gate="1" pin="1Q" pad="19"/>
<connect gate="1" pin="2D" pad="3"/>
<connect gate="1" pin="2Q" pad="18"/>
<connect gate="1" pin="3D" pad="4"/>
<connect gate="1" pin="3Q" pad="17"/>
<connect gate="1" pin="4D" pad="5"/>
<connect gate="1" pin="4Q" pad="16"/>
<connect gate="1" pin="5D" pad="6"/>
<connect gate="1" pin="5Q" pad="15"/>
<connect gate="1" pin="6D" pad="7"/>
<connect gate="1" pin="6Q" pad="14"/>
<connect gate="1" pin="7D" pad="8"/>
<connect gate="1" pin="7Q" pad="13"/>
<connect gate="1" pin="8D" pad="9"/>
<connect gate="1" pin="8Q" pad="12"/>
<connect gate="1" pin="C" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*574" prefix="V">
<description>8-bit D type &lt;b&gt;FLIP FLOP&lt;/b&gt; bus driver</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="574"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!OC" pad="1"/>
<connect gate="1" pin="1D" pad="2"/>
<connect gate="1" pin="1Q" pad="19"/>
<connect gate="1" pin="2D" pad="3"/>
<connect gate="1" pin="2Q" pad="18"/>
<connect gate="1" pin="3D" pad="4"/>
<connect gate="1" pin="3Q" pad="17"/>
<connect gate="1" pin="4D" pad="5"/>
<connect gate="1" pin="4Q" pad="16"/>
<connect gate="1" pin="5D" pad="6"/>
<connect gate="1" pin="5Q" pad="15"/>
<connect gate="1" pin="6D" pad="7"/>
<connect gate="1" pin="6Q" pad="14"/>
<connect gate="1" pin="7D" pad="8"/>
<connect gate="1" pin="7Q" pad="13"/>
<connect gate="1" pin="8D" pad="9"/>
<connect gate="1" pin="8Q" pad="12"/>
<connect gate="1" pin="CLK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*590A" prefix="V">
<description>8-bit &lt;b&gt;BINARY COUNTER&lt;/b&gt; with output register</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="590A"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CCKEN" pad="12"/>
<connect gate="1" pin="!CCLR" pad="10"/>
<connect gate="1" pin="!G" pad="14"/>
<connect gate="1" pin="!RCO" pad="9"/>
<connect gate="1" pin="CCK" pad="11"/>
<connect gate="1" pin="QA" pad="15"/>
<connect gate="1" pin="QB" pad="1"/>
<connect gate="1" pin="QC" pad="2"/>
<connect gate="1" pin="QD" pad="3"/>
<connect gate="1" pin="QE" pad="4"/>
<connect gate="1" pin="QF" pad="5"/>
<connect gate="1" pin="QG" pad="6"/>
<connect gate="1" pin="QH" pad="7"/>
<connect gate="1" pin="RCK" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*594" prefix="V">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="594"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!RCLR" pad="13"/>
<connect gate="1" pin="!SRCLR" pad="10"/>
<connect gate="1" pin="QA" pad="15"/>
<connect gate="1" pin="QB" pad="1"/>
<connect gate="1" pin="QC" pad="2"/>
<connect gate="1" pin="QD" pad="3"/>
<connect gate="1" pin="QE" pad="4"/>
<connect gate="1" pin="QF" pad="5"/>
<connect gate="1" pin="QG" pad="6"/>
<connect gate="1" pin="QH" pad="7"/>
<connect gate="1" pin="QH*" pad="9"/>
<connect gate="1" pin="RCK" pad="12"/>
<connect gate="1" pin="SER" pad="14"/>
<connect gate="1" pin="SRCK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*595" prefix="V">
<description>8-bit &lt;b&gt;SHIFT REGISTER&lt;/b&gt;, output latch</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="595"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G" pad="13"/>
<connect gate="1" pin="!SRCLR" pad="10"/>
<connect gate="1" pin="QA" pad="15"/>
<connect gate="1" pin="QB" pad="1"/>
<connect gate="1" pin="QC" pad="2"/>
<connect gate="1" pin="QD" pad="3"/>
<connect gate="1" pin="QE" pad="4"/>
<connect gate="1" pin="QF" pad="5"/>
<connect gate="1" pin="QG" pad="6"/>
<connect gate="1" pin="QH" pad="7"/>
<connect gate="1" pin="QH*" pad="9"/>
<connect gate="1" pin="RCK" pad="12"/>
<connect gate="1" pin="SER" pad="14"/>
<connect gate="1" pin="SRCK" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4002" prefix="V">
<description>Dual 4-input &lt;b&gt;NOR&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="4002"/>
<gate name="/2" symbol="4002"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="2"/>
<connect gate="/1" pin="B" pad="3"/>
<connect gate="/1" pin="C" pad="4"/>
<connect gate="/1" pin="D" pad="5"/>
<connect gate="/1" pin="Y" pad="1"/>
<connect gate="/2" pin="A" pad="9"/>
<connect gate="/2" pin="B" pad="10"/>
<connect gate="/2" pin="C" pad="11"/>
<connect gate="/2" pin="D" pad="12"/>
<connect gate="/2" pin="Y" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="54*4016" prefix="V">
<description>Quad analog &lt;b&gt;switch&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="4016"/>
<gate name="/2" symbol="4016"/>
<gate name="/3" symbol="4016"/>
<gate name="/4" symbol="4016"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="C" pad="13"/>
<connect gate="/2" pin="A" pad="11"/>
<connect gate="/2" pin="B" pad="10"/>
<connect gate="/2" pin="C" pad="12"/>
<connect gate="/3" pin="A" pad="4"/>
<connect gate="/3" pin="B" pad="3"/>
<connect gate="/3" pin="C" pad="5"/>
<connect gate="/4" pin="A" pad="8"/>
<connect gate="/4" pin="B" pad="9"/>
<connect gate="/4" pin="C" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4017" prefix="V">
<description>4-bit asynchronous decade &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4017"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLKEN" pad="13"/>
<connect gate="1" pin="CLK" pad="14"/>
<connect gate="1" pin="CLR" pad="15"/>
<connect gate="1" pin="CO" pad="12"/>
<connect gate="1" pin="Y0" pad="3"/>
<connect gate="1" pin="Y1" pad="2"/>
<connect gate="1" pin="Y2" pad="4"/>
<connect gate="1" pin="Y3" pad="7"/>
<connect gate="1" pin="Y4" pad="10"/>
<connect gate="1" pin="Y5" pad="1"/>
<connect gate="1" pin="Y6" pad="5"/>
<connect gate="1" pin="Y7" pad="6"/>
<connect gate="1" pin="Y8" pad="9"/>
<connect gate="1" pin="Y9" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4020" prefix="V">
<description>14-bit asynchronous binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4020"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="CLK" pad="10"/>
<connect gate="1" pin="CLR" pad="11"/>
<connect gate="1" pin="QA" pad="9"/>
<connect gate="1" pin="QD" pad="7"/>
<connect gate="1" pin="QE" pad="5"/>
<connect gate="1" pin="QF" pad="4"/>
<connect gate="1" pin="QG" pad="6"/>
<connect gate="1" pin="QH" pad="13"/>
<connect gate="1" pin="QI" pad="12"/>
<connect gate="1" pin="QJ" pad="14"/>
<connect gate="1" pin="QK" pad="15"/>
<connect gate="1" pin="QL" pad="1"/>
<connect gate="1" pin="QM" pad="2"/>
<connect gate="1" pin="QN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4024" prefix="V">
<description>7-bit asynchronous binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4024"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="CLK" pad="1"/>
<connect gate="1" pin="CLR" pad="2"/>
<connect gate="1" pin="QA" pad="12"/>
<connect gate="1" pin="QB" pad="11"/>
<connect gate="1" pin="QC" pad="9"/>
<connect gate="1" pin="QD" pad="6"/>
<connect gate="1" pin="QE" pad="5"/>
<connect gate="1" pin="QF" pad="4"/>
<connect gate="1" pin="QG" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4040" prefix="V">
<description>12-bit asynchronous binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4040"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="CLK" pad="10"/>
<connect gate="1" pin="CLR" pad="11"/>
<connect gate="1" pin="QA" pad="9"/>
<connect gate="1" pin="QB" pad="7"/>
<connect gate="1" pin="QC" pad="6"/>
<connect gate="1" pin="QD" pad="5"/>
<connect gate="1" pin="QE" pad="3"/>
<connect gate="1" pin="QF" pad="2"/>
<connect gate="1" pin="QG" pad="4"/>
<connect gate="1" pin="QH" pad="13"/>
<connect gate="1" pin="QI" pad="12"/>
<connect gate="1" pin="QJ" pad="14"/>
<connect gate="1" pin="QK" pad="15"/>
<connect gate="1" pin="QL" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4060" prefix="V">
<description>14-bit asynchronous binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4060"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CKO" pad="10"/>
<connect gate="1" pin="CKI" pad="11"/>
<connect gate="1" pin="CKO" pad="9"/>
<connect gate="1" pin="CLR" pad="12"/>
<connect gate="1" pin="QD" pad="7"/>
<connect gate="1" pin="QE" pad="5"/>
<connect gate="1" pin="QF" pad="4"/>
<connect gate="1" pin="QG" pad="6"/>
<connect gate="1" pin="QH" pad="14"/>
<connect gate="1" pin="QI" pad="13"/>
<connect gate="1" pin="QJ" pad="15"/>
<connect gate="1" pin="QL" pad="1"/>
<connect gate="1" pin="QM" pad="2"/>
<connect gate="1" pin="QN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4061" prefix="V">
<description>14-bit asynchronous binary &lt;b&gt;COUNTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4061"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CKO" pad="10"/>
<connect gate="1" pin="CKI" pad="11"/>
<connect gate="1" pin="CKO" pad="9"/>
<connect gate="1" pin="CLR" pad="12"/>
<connect gate="1" pin="QD" pad="7"/>
<connect gate="1" pin="QE" pad="5"/>
<connect gate="1" pin="QF" pad="4"/>
<connect gate="1" pin="QG" pad="6"/>
<connect gate="1" pin="QH" pad="14"/>
<connect gate="1" pin="QI" pad="13"/>
<connect gate="1" pin="QJ" pad="15"/>
<connect gate="1" pin="QL" pad="1"/>
<connect gate="1" pin="QM" pad="2"/>
<connect gate="1" pin="QN" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4066" prefix="V">
<description>Quad analog &lt;b&gt;SWITCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="4066"/>
<gate name="/2" symbol="4066"/>
<gate name="/3" symbol="4066"/>
<gate name="/4" symbol="4066"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="C" pad="13"/>
<connect gate="/2" pin="A" pad="11"/>
<connect gate="/2" pin="B" pad="10"/>
<connect gate="/2" pin="C" pad="12"/>
<connect gate="/3" pin="A" pad="4"/>
<connect gate="/3" pin="B" pad="3"/>
<connect gate="/3" pin="C" pad="5"/>
<connect gate="/4" pin="A" pad="8"/>
<connect gate="/4" pin="B" pad="9"/>
<connect gate="/4" pin="C" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4075" prefix="V">
<description>Triple 3-input &lt;b&gt;OR&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="4075"/>
<gate name="/2" symbol="4075"/>
<gate name="/3" symbol="4075"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="C" pad="8"/>
<connect gate="/1" pin="Y" pad="9"/>
<connect gate="/2" pin="A" pad="3"/>
<connect gate="/2" pin="B" pad="4"/>
<connect gate="/2" pin="C" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="11"/>
<connect gate="/3" pin="B" pad="12"/>
<connect gate="/3" pin="C" pad="13"/>
<connect gate="/3" pin="Y" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4078" prefix="V">
<description>8-input &lt;b&gt;OR/NOR&lt;/b&gt;, complementary outputs</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4078"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="1" pin="A" pad="2"/>
<connect gate="1" pin="B" pad="3"/>
<connect gate="1" pin="C" pad="4"/>
<connect gate="1" pin="D" pad="5"/>
<connect gate="1" pin="E" pad="9"/>
<connect gate="1" pin="F" pad="10"/>
<connect gate="1" pin="G" pad="11"/>
<connect gate="1" pin="H" pad="12"/>
<connect gate="1" pin="W" pad="13"/>
<connect gate="1" pin="Y" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4514" prefix="V">
<description>1 of 16 noninverting &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4514"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!G" pad="23"/>
<connect gate="1" pin="A" pad="2"/>
<connect gate="1" pin="B" pad="3"/>
<connect gate="1" pin="C" pad="21"/>
<connect gate="1" pin="D" pad="22"/>
<connect gate="1" pin="LE" pad="1"/>
<connect gate="1" pin="Y0" pad="11"/>
<connect gate="1" pin="Y1" pad="10"/>
<connect gate="1" pin="Y10" pad="20"/>
<connect gate="1" pin="Y11" pad="19"/>
<connect gate="1" pin="Y12" pad="14"/>
<connect gate="1" pin="Y13" pad="13"/>
<connect gate="1" pin="Y14" pad="16"/>
<connect gate="1" pin="Y15" pad="15"/>
<connect gate="1" pin="Y2" pad="9"/>
<connect gate="1" pin="Y3" pad="8"/>
<connect gate="1" pin="Y4" pad="7"/>
<connect gate="1" pin="Y5" pad="6"/>
<connect gate="1" pin="Y6" pad="5"/>
<connect gate="1" pin="Y7" pad="4"/>
<connect gate="1" pin="Y8" pad="18"/>
<connect gate="1" pin="Y9" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4515" prefix="V">
<description>1 of 16 inverting &lt;b&gt;DECODER/DEMULTIPLEXER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4515"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!G" pad="23"/>
<connect gate="1" pin="A" pad="2"/>
<connect gate="1" pin="B" pad="3"/>
<connect gate="1" pin="C" pad="21"/>
<connect gate="1" pin="D" pad="22"/>
<connect gate="1" pin="LE" pad="1"/>
<connect gate="1" pin="Y0" pad="11"/>
<connect gate="1" pin="Y1" pad="10"/>
<connect gate="1" pin="Y10" pad="20"/>
<connect gate="1" pin="Y11" pad="19"/>
<connect gate="1" pin="Y12" pad="14"/>
<connect gate="1" pin="Y13" pad="13"/>
<connect gate="1" pin="Y14" pad="16"/>
<connect gate="1" pin="Y15" pad="15"/>
<connect gate="1" pin="Y2" pad="9"/>
<connect gate="1" pin="Y3" pad="8"/>
<connect gate="1" pin="Y4" pad="7"/>
<connect gate="1" pin="Y5" pad="6"/>
<connect gate="1" pin="Y6" pad="5"/>
<connect gate="1" pin="Y7" pad="4"/>
<connect gate="1" pin="Y8" pad="18"/>
<connect gate="1" pin="Y9" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4724" prefix="V">
<description>8 Bit Addressable &lt;b&gt;LATCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="4724"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!G" pad="14"/>
<connect gate="1" pin="CLR" pad="15"/>
<connect gate="1" pin="D" pad="13"/>
<connect gate="1" pin="Q0" pad="4"/>
<connect gate="1" pin="Q1" pad="5"/>
<connect gate="1" pin="Q2" pad="6"/>
<connect gate="1" pin="Q3" pad="7"/>
<connect gate="1" pin="Q4" pad="9"/>
<connect gate="1" pin="Q5" pad="10"/>
<connect gate="1" pin="Q6" pad="11"/>
<connect gate="1" pin="Q7" pad="12"/>
<connect gate="1" pin="S0" pad="1"/>
<connect gate="1" pin="S1" pad="2"/>
<connect gate="1" pin="S2" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*604" prefix="V">
<description>Octal 2-input &lt;b&gt;MULTIPLEXED LATCH&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="604"/>
</gates>
<devices>
<device name="N" package="DIL28-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="28"/>
<connect gate="/-UB" pin="-UB" pad="14"/>
<connect gate="1" pin="A1" pad="3"/>
<connect gate="1" pin="A2" pad="5"/>
<connect gate="1" pin="A3" pad="7"/>
<connect gate="1" pin="A4" pad="9"/>
<connect gate="1" pin="A5" pad="27"/>
<connect gate="1" pin="A6" pad="25"/>
<connect gate="1" pin="A7" pad="23"/>
<connect gate="1" pin="A8" pad="21"/>
<connect gate="1" pin="B1" pad="4"/>
<connect gate="1" pin="B2" pad="6"/>
<connect gate="1" pin="B3" pad="8"/>
<connect gate="1" pin="B4" pad="10"/>
<connect gate="1" pin="B5" pad="26"/>
<connect gate="1" pin="B6" pad="24"/>
<connect gate="1" pin="B7" pad="22"/>
<connect gate="1" pin="B8" pad="20"/>
<connect gate="1" pin="CLK" pad="1"/>
<connect gate="1" pin="SEL_A/!B" pad="2"/>
<connect gate="1" pin="Y1" pad="15"/>
<connect gate="1" pin="Y2" pad="13"/>
<connect gate="1" pin="Y3" pad="12"/>
<connect gate="1" pin="Y4" pad="11"/>
<connect gate="1" pin="Y5" pad="16"/>
<connect gate="1" pin="Y6" pad="17"/>
<connect gate="1" pin="Y7" pad="18"/>
<connect gate="1" pin="Y8" pad="19"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*620" prefix="V">
<description>Octal &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="620"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!GBA" pad="19"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="B1" pad="18"/>
<connect gate="1" pin="B2" pad="17"/>
<connect gate="1" pin="B3" pad="16"/>
<connect gate="1" pin="B4" pad="15"/>
<connect gate="1" pin="B5" pad="14"/>
<connect gate="1" pin="B6" pad="13"/>
<connect gate="1" pin="B7" pad="12"/>
<connect gate="1" pin="B8" pad="11"/>
<connect gate="1" pin="GAB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*623" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="623"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!GBA" pad="19"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="B1" pad="18"/>
<connect gate="1" pin="B2" pad="17"/>
<connect gate="1" pin="B3" pad="16"/>
<connect gate="1" pin="B4" pad="15"/>
<connect gate="1" pin="B5" pad="14"/>
<connect gate="1" pin="B6" pad="13"/>
<connect gate="1" pin="B7" pad="12"/>
<connect gate="1" pin="B8" pad="11"/>
<connect gate="1" pin="GAB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*640" prefix="V">
<description>Octal bus &lt;B&gt;TRANSCEIVER&lt;/B&gt; 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="640"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G" pad="19"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="B1" pad="18"/>
<connect gate="1" pin="B2" pad="17"/>
<connect gate="1" pin="B3" pad="16"/>
<connect gate="1" pin="B4" pad="15"/>
<connect gate="1" pin="B5" pad="14"/>
<connect gate="1" pin="B6" pad="13"/>
<connect gate="1" pin="B7" pad="12"/>
<connect gate="1" pin="B8" pad="11"/>
<connect gate="1" pin="DIR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*643" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt; 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="643"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G" pad="19"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="B1" pad="18"/>
<connect gate="1" pin="B2" pad="17"/>
<connect gate="1" pin="B3" pad="16"/>
<connect gate="1" pin="B4" pad="15"/>
<connect gate="1" pin="B5" pad="14"/>
<connect gate="1" pin="B6" pad="13"/>
<connect gate="1" pin="B7" pad="12"/>
<connect gate="1" pin="B8" pad="11"/>
<connect gate="1" pin="DIR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*645" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt; 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="645"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G" pad="19"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="B1" pad="18"/>
<connect gate="1" pin="B2" pad="17"/>
<connect gate="1" pin="B3" pad="16"/>
<connect gate="1" pin="B4" pad="15"/>
<connect gate="1" pin="B5" pad="14"/>
<connect gate="1" pin="B6" pad="13"/>
<connect gate="1" pin="B7" pad="12"/>
<connect gate="1" pin="B8" pad="11"/>
<connect gate="1" pin="DIR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*646" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="646"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!G" pad="21"/>
<connect gate="1" pin="A1" pad="4"/>
<connect gate="1" pin="A2" pad="5"/>
<connect gate="1" pin="A3" pad="6"/>
<connect gate="1" pin="A4" pad="7"/>
<connect gate="1" pin="A5" pad="8"/>
<connect gate="1" pin="A6" pad="9"/>
<connect gate="1" pin="A7" pad="10"/>
<connect gate="1" pin="A8" pad="11"/>
<connect gate="1" pin="B1" pad="20"/>
<connect gate="1" pin="B2" pad="19"/>
<connect gate="1" pin="B3" pad="18"/>
<connect gate="1" pin="B4" pad="17"/>
<connect gate="1" pin="B5" pad="16"/>
<connect gate="1" pin="B6" pad="15"/>
<connect gate="1" pin="B7" pad="14"/>
<connect gate="1" pin="B8" pad="13"/>
<connect gate="1" pin="CAB" pad="1"/>
<connect gate="1" pin="CBA" pad="23"/>
<connect gate="1" pin="DIR" pad="3"/>
<connect gate="1" pin="SAB" pad="2"/>
<connect gate="1" pin="SBA" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*648" prefix="V">
<description>8-bit inverting &lt;b&gt;TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="648"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!G" pad="21"/>
<connect gate="1" pin="A1" pad="4"/>
<connect gate="1" pin="A2" pad="5"/>
<connect gate="1" pin="A3" pad="6"/>
<connect gate="1" pin="A4" pad="7"/>
<connect gate="1" pin="A5" pad="8"/>
<connect gate="1" pin="A6" pad="9"/>
<connect gate="1" pin="A7" pad="10"/>
<connect gate="1" pin="A8" pad="11"/>
<connect gate="1" pin="B1" pad="20"/>
<connect gate="1" pin="B2" pad="19"/>
<connect gate="1" pin="B3" pad="18"/>
<connect gate="1" pin="B4" pad="17"/>
<connect gate="1" pin="B5" pad="16"/>
<connect gate="1" pin="B6" pad="15"/>
<connect gate="1" pin="B7" pad="14"/>
<connect gate="1" pin="B8" pad="13"/>
<connect gate="1" pin="CAB" pad="1"/>
<connect gate="1" pin="CBA" pad="23"/>
<connect gate="1" pin="DIR" pad="3"/>
<connect gate="1" pin="SAB" pad="2"/>
<connect gate="1" pin="SBA" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*651" prefix="V">
<description>8-bit &lt;b&gt;BUS TRANSCEIVER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="651"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!GBA" pad="21"/>
<connect gate="1" pin="A1" pad="4"/>
<connect gate="1" pin="A2" pad="5"/>
<connect gate="1" pin="A3" pad="6"/>
<connect gate="1" pin="A4" pad="7"/>
<connect gate="1" pin="A5" pad="8"/>
<connect gate="1" pin="A6" pad="9"/>
<connect gate="1" pin="A7" pad="10"/>
<connect gate="1" pin="A8" pad="11"/>
<connect gate="1" pin="B1" pad="20"/>
<connect gate="1" pin="B2" pad="19"/>
<connect gate="1" pin="B3" pad="18"/>
<connect gate="1" pin="B4" pad="17"/>
<connect gate="1" pin="B5" pad="16"/>
<connect gate="1" pin="B6" pad="15"/>
<connect gate="1" pin="B7" pad="14"/>
<connect gate="1" pin="B8" pad="13"/>
<connect gate="1" pin="CAB" pad="1"/>
<connect gate="1" pin="CBA" pad="23"/>
<connect gate="1" pin="GAB" pad="3"/>
<connect gate="1" pin="SAB" pad="2"/>
<connect gate="1" pin="SBA" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*652" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="652"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!GBA" pad="21"/>
<connect gate="1" pin="A1" pad="4"/>
<connect gate="1" pin="A2" pad="5"/>
<connect gate="1" pin="A3" pad="6"/>
<connect gate="1" pin="A4" pad="7"/>
<connect gate="1" pin="A5" pad="8"/>
<connect gate="1" pin="A6" pad="9"/>
<connect gate="1" pin="A7" pad="10"/>
<connect gate="1" pin="A8" pad="11"/>
<connect gate="1" pin="B1" pad="20"/>
<connect gate="1" pin="B2" pad="19"/>
<connect gate="1" pin="B3" pad="18"/>
<connect gate="1" pin="B4" pad="17"/>
<connect gate="1" pin="B5" pad="16"/>
<connect gate="1" pin="B6" pad="15"/>
<connect gate="1" pin="B7" pad="14"/>
<connect gate="1" pin="B8" pad="13"/>
<connect gate="1" pin="CAB" pad="1"/>
<connect gate="1" pin="CBA" pad="23"/>
<connect gate="1" pin="GAB" pad="3"/>
<connect gate="1" pin="SAB" pad="2"/>
<connect gate="1" pin="SBA" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*658" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="658"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!GBA" pad="23"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="API" pad="14"/>
<connect gate="1" pin="APO" pad="13"/>
<connect gate="1" pin="B1" pad="22"/>
<connect gate="1" pin="B2" pad="21"/>
<connect gate="1" pin="B3" pad="20"/>
<connect gate="1" pin="B4" pad="19"/>
<connect gate="1" pin="B5" pad="18"/>
<connect gate="1" pin="B6" pad="17"/>
<connect gate="1" pin="B7" pad="16"/>
<connect gate="1" pin="B8" pad="15"/>
<connect gate="1" pin="BPI" pad="10"/>
<connect gate="1" pin="BPO" pad="11"/>
<connect gate="1" pin="GAB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*659" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt;, 3-state</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="659"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!GBA" pad="23"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="API" pad="14"/>
<connect gate="1" pin="APO" pad="13"/>
<connect gate="1" pin="B1" pad="22"/>
<connect gate="1" pin="B2" pad="21"/>
<connect gate="1" pin="B3" pad="20"/>
<connect gate="1" pin="B4" pad="19"/>
<connect gate="1" pin="B5" pad="18"/>
<connect gate="1" pin="B6" pad="17"/>
<connect gate="1" pin="B7" pad="16"/>
<connect gate="1" pin="B8" pad="15"/>
<connect gate="1" pin="BPI" pad="10"/>
<connect gate="1" pin="BPO" pad="11"/>
<connect gate="1" pin="GAB" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*664" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt;, parity</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="664"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!G" pad="23"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="API" pad="14"/>
<connect gate="1" pin="APO" pad="13"/>
<connect gate="1" pin="B1" pad="22"/>
<connect gate="1" pin="B2" pad="21"/>
<connect gate="1" pin="B3" pad="20"/>
<connect gate="1" pin="B4" pad="19"/>
<connect gate="1" pin="B5" pad="18"/>
<connect gate="1" pin="B6" pad="17"/>
<connect gate="1" pin="B7" pad="16"/>
<connect gate="1" pin="B8" pad="15"/>
<connect gate="1" pin="BPI" pad="10"/>
<connect gate="1" pin="BPO" pad="11"/>
<connect gate="1" pin="DIR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*665" prefix="V">
<description>Octal bus &lt;b&gt;TRANSCEIVER&lt;/b&gt;, parity</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="665"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!G" pad="23"/>
<connect gate="1" pin="A1" pad="2"/>
<connect gate="1" pin="A2" pad="3"/>
<connect gate="1" pin="A3" pad="4"/>
<connect gate="1" pin="A4" pad="5"/>
<connect gate="1" pin="A5" pad="6"/>
<connect gate="1" pin="A6" pad="7"/>
<connect gate="1" pin="A7" pad="8"/>
<connect gate="1" pin="A8" pad="9"/>
<connect gate="1" pin="API" pad="14"/>
<connect gate="1" pin="APO" pad="13"/>
<connect gate="1" pin="B1" pad="22"/>
<connect gate="1" pin="B2" pad="21"/>
<connect gate="1" pin="B3" pad="20"/>
<connect gate="1" pin="B4" pad="19"/>
<connect gate="1" pin="B5" pad="18"/>
<connect gate="1" pin="B6" pad="17"/>
<connect gate="1" pin="B7" pad="16"/>
<connect gate="1" pin="B8" pad="15"/>
<connect gate="1" pin="BPI" pad="10"/>
<connect gate="1" pin="BPO" pad="11"/>
<connect gate="1" pin="DIR" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*677" prefix="V">
<description>16-bit address &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="677"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="!G" pad="23"/>
<connect gate="1" pin="A1" pad="1"/>
<connect gate="1" pin="A10" pad="10"/>
<connect gate="1" pin="A11" pad="11"/>
<connect gate="1" pin="A12" pad="13"/>
<connect gate="1" pin="A13" pad="14"/>
<connect gate="1" pin="A14" pad="15"/>
<connect gate="1" pin="A15" pad="16"/>
<connect gate="1" pin="A16" pad="17"/>
<connect gate="1" pin="A2" pad="2"/>
<connect gate="1" pin="A3" pad="3"/>
<connect gate="1" pin="A4" pad="4"/>
<connect gate="1" pin="A5" pad="5"/>
<connect gate="1" pin="A6" pad="6"/>
<connect gate="1" pin="A7" pad="7"/>
<connect gate="1" pin="A8" pad="8"/>
<connect gate="1" pin="A9" pad="9"/>
<connect gate="1" pin="P0" pad="18"/>
<connect gate="1" pin="P1" pad="19"/>
<connect gate="1" pin="P2" pad="20"/>
<connect gate="1" pin="P3" pad="21"/>
<connect gate="1" pin="Y" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*678" prefix="V">
<description>16-bit address &lt;b&gt;COMPARATOR&lt;/b&gt;, latch</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="678"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="1" pin="A1" pad="1"/>
<connect gate="1" pin="A10" pad="10"/>
<connect gate="1" pin="A11" pad="11"/>
<connect gate="1" pin="A12" pad="13"/>
<connect gate="1" pin="A13" pad="14"/>
<connect gate="1" pin="A14" pad="15"/>
<connect gate="1" pin="A15" pad="16"/>
<connect gate="1" pin="A16" pad="17"/>
<connect gate="1" pin="A2" pad="2"/>
<connect gate="1" pin="A3" pad="3"/>
<connect gate="1" pin="A4" pad="4"/>
<connect gate="1" pin="A5" pad="5"/>
<connect gate="1" pin="A6" pad="6"/>
<connect gate="1" pin="A7" pad="7"/>
<connect gate="1" pin="A8" pad="8"/>
<connect gate="1" pin="A9" pad="9"/>
<connect gate="1" pin="C" pad="23"/>
<connect gate="1" pin="P0" pad="18"/>
<connect gate="1" pin="P1" pad="19"/>
<connect gate="1" pin="P2" pad="20"/>
<connect gate="1" pin="P3" pad="21"/>
<connect gate="1" pin="Y" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*679" prefix="V">
<description>12-bit address &lt;b&gt;COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="679"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G" pad="19"/>
<connect gate="1" pin="A1" pad="1"/>
<connect gate="1" pin="A10" pad="11"/>
<connect gate="1" pin="A11" pad="12"/>
<connect gate="1" pin="A12" pad="13"/>
<connect gate="1" pin="A2" pad="2"/>
<connect gate="1" pin="A3" pad="3"/>
<connect gate="1" pin="A4" pad="4"/>
<connect gate="1" pin="A5" pad="5"/>
<connect gate="1" pin="A6" pad="6"/>
<connect gate="1" pin="A7" pad="7"/>
<connect gate="1" pin="A8" pad="8"/>
<connect gate="1" pin="A9" pad="9"/>
<connect gate="1" pin="P0" pad="14"/>
<connect gate="1" pin="P1" pad="15"/>
<connect gate="1" pin="P2" pad="16"/>
<connect gate="1" pin="P3" pad="17"/>
<connect gate="1" pin="Y" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*680" prefix="V">
<description>12-bit address &lt;b&gt;COMPARATOR&lt;/b&gt;, latch</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="680"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="A1" pad="1"/>
<connect gate="1" pin="A10" pad="11"/>
<connect gate="1" pin="A11" pad="12"/>
<connect gate="1" pin="A12" pad="13"/>
<connect gate="1" pin="A2" pad="2"/>
<connect gate="1" pin="A3" pad="3"/>
<connect gate="1" pin="A4" pad="4"/>
<connect gate="1" pin="A5" pad="5"/>
<connect gate="1" pin="A6" pad="6"/>
<connect gate="1" pin="A7" pad="7"/>
<connect gate="1" pin="A8" pad="8"/>
<connect gate="1" pin="A9" pad="9"/>
<connect gate="1" pin="C" pad="19"/>
<connect gate="1" pin="P0" pad="14"/>
<connect gate="1" pin="P1" pad="15"/>
<connect gate="1" pin="P2" pad="16"/>
<connect gate="1" pin="P3" pad="17"/>
<connect gate="1" pin="Y" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*682" prefix="V">
<description>8-bit &lt;b&gt;MAGNITUDE/IDENTITY COMPARATOR&lt;/b&gt;, totem pole</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="682"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!P=Q" pad="19"/>
<connect gate="1" pin="!P&gt;Q" pad="1"/>
<connect gate="1" pin="P0" pad="2"/>
<connect gate="1" pin="P1" pad="4"/>
<connect gate="1" pin="P2" pad="6"/>
<connect gate="1" pin="P3" pad="8"/>
<connect gate="1" pin="P4" pad="11"/>
<connect gate="1" pin="P5" pad="13"/>
<connect gate="1" pin="P6" pad="15"/>
<connect gate="1" pin="P7" pad="17"/>
<connect gate="1" pin="Q0" pad="3"/>
<connect gate="1" pin="Q1" pad="5"/>
<connect gate="1" pin="Q2" pad="7"/>
<connect gate="1" pin="Q3" pad="9"/>
<connect gate="1" pin="Q4" pad="12"/>
<connect gate="1" pin="Q5" pad="14"/>
<connect gate="1" pin="Q6" pad="16"/>
<connect gate="1" pin="Q7" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*684" prefix="V">
<description>8-bit &lt;b&gt;MAGNITUDE COMPARATOR&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="684"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!P=Q" pad="19"/>
<connect gate="1" pin="!P&gt;Q" pad="1"/>
<connect gate="1" pin="P0" pad="2"/>
<connect gate="1" pin="P1" pad="4"/>
<connect gate="1" pin="P2" pad="6"/>
<connect gate="1" pin="P3" pad="8"/>
<connect gate="1" pin="P4" pad="11"/>
<connect gate="1" pin="P5" pad="13"/>
<connect gate="1" pin="P6" pad="15"/>
<connect gate="1" pin="P7" pad="17"/>
<connect gate="1" pin="Q0" pad="3"/>
<connect gate="1" pin="Q1" pad="5"/>
<connect gate="1" pin="Q2" pad="7"/>
<connect gate="1" pin="Q3" pad="9"/>
<connect gate="1" pin="Q4" pad="12"/>
<connect gate="1" pin="Q5" pad="14"/>
<connect gate="1" pin="Q6" pad="16"/>
<connect gate="1" pin="Q7" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*688" prefix="V">
<description>8-bit &lt;b&gt;MAGNITUDE/IDENTITY COMPARATOR&lt;/b&gt;, totem pole</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="688"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="1" pin="!G" pad="1"/>
<connect gate="1" pin="!P=Q" pad="19"/>
<connect gate="1" pin="P0" pad="2"/>
<connect gate="1" pin="P1" pad="4"/>
<connect gate="1" pin="P2" pad="6"/>
<connect gate="1" pin="P3" pad="8"/>
<connect gate="1" pin="P4" pad="11"/>
<connect gate="1" pin="P5" pad="13"/>
<connect gate="1" pin="P6" pad="15"/>
<connect gate="1" pin="P7" pad="17"/>
<connect gate="1" pin="Q0" pad="3"/>
<connect gate="1" pin="Q1" pad="5"/>
<connect gate="1" pin="Q2" pad="7"/>
<connect gate="1" pin="Q3" pad="9"/>
<connect gate="1" pin="Q4" pad="12"/>
<connect gate="1" pin="Q5" pad="14"/>
<connect gate="1" pin="Q6" pad="16"/>
<connect gate="1" pin="Q7" pad="18"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7001" prefix="V">
<description>Quad 2-input &lt;b&gt;AND&lt;/b&gt;, schmitt trigger</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7001"/>
<gate name="/2" symbol="7001"/>
<gate name="/3" symbol="7001"/>
<gate name="/4" symbol="7001"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7002" prefix="V">
<description>Quad &lt;b&gt;NOR&lt;/b&gt;, schmitt trigger</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7002"/>
<gate name="/2" symbol="7002"/>
<gate name="/3" symbol="7002"/>
<gate name="/4" symbol="7002"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7006" prefix="V">
<description>&lt;b&gt;NOR/NAND/INVERTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7006_6"/>
<gate name="/2" symbol="7006_5"/>
<gate name="/3" symbol="7006_4"/>
<gate name="/4" symbol="7006_3"/>
<gate name="/5" symbol="7006_2"/>
<gate name="/6" symbol="7006_1"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="/1" pin="A" pad="19"/>
<connect gate="/1" pin="B" pad="20"/>
<connect gate="/1" pin="C" pad="22"/>
<connect gate="/1" pin="D" pad="23"/>
<connect gate="/1" pin="Y" pad="21"/>
<connect gate="/2" pin="A" pad="16"/>
<connect gate="/2" pin="B" pad="17"/>
<connect gate="/2" pin="C" pad="18"/>
<connect gate="/2" pin="Y" pad="15"/>
<connect gate="/3" pin="A" pad="13"/>
<connect gate="/3" pin="Y" pad="14"/>
<connect gate="/4" pin="A" pad="11"/>
<connect gate="/4" pin="Y" pad="10"/>
<connect gate="/5" pin="A" pad="6"/>
<connect gate="/5" pin="B" pad="7"/>
<connect gate="/5" pin="C" pad="8"/>
<connect gate="/5" pin="Y" pad="9"/>
<connect gate="/6" pin="A" pad="1"/>
<connect gate="/6" pin="B" pad="2"/>
<connect gate="/6" pin="C" pad="4"/>
<connect gate="/6" pin="D" pad="5"/>
<connect gate="/6" pin="Y" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7008" prefix="V">
<description>&lt;b&gt;NOR/NAND/INVERTER&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7008_8"/>
<gate name="/2" symbol="7008_7"/>
<gate name="/3" symbol="7008_6"/>
<gate name="/4" symbol="7008_5"/>
<gate name="/5" symbol="7008_4"/>
<gate name="/6" symbol="7008_3"/>
<gate name="/7" symbol="7008_2"/>
<gate name="/8" symbol="7008_1"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="/1" pin="A" pad="22"/>
<connect gate="/1" pin="B" pad="23"/>
<connect gate="/1" pin="Y" pad="21"/>
<connect gate="/2" pin="A" pad="18"/>
<connect gate="/2" pin="B" pad="19"/>
<connect gate="/2" pin="Y" pad="20"/>
<connect gate="/3" pin="A" pad="16"/>
<connect gate="/3" pin="B" pad="17"/>
<connect gate="/3" pin="Y" pad="15"/>
<connect gate="/4" pin="A" pad="13"/>
<connect gate="/4" pin="Y" pad="14"/>
<connect gate="/5" pin="A" pad="11"/>
<connect gate="/5" pin="Y" pad="10"/>
<connect gate="/6" pin="A" pad="7"/>
<connect gate="/6" pin="B" pad="8"/>
<connect gate="/6" pin="Y" pad="9"/>
<connect gate="/7" pin="A" pad="5"/>
<connect gate="/7" pin="B" pad="6"/>
<connect gate="/7" pin="Y" pad="4"/>
<connect gate="/8" pin="A" pad="1"/>
<connect gate="/8" pin="B" pad="2"/>
<connect gate="/8" pin="Y" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7022" prefix="V">
<description>Octal &lt;b&gt;COUNTER/DIVIDER&lt;/b&gt; with 1-of-8 Decoded Outputs</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="1" symbol="7022"/>
</gates>
<devices>
<device name="N" package="DIL16">
<connects>
<connect gate="/+UB" pin="+UB" pad="16"/>
<connect gate="/-UB" pin="-UB" pad="8"/>
<connect gate="1" pin="!CLKEN" pad="13"/>
<connect gate="1" pin="!CLROUT" pad="9"/>
<connect gate="1" pin="CLK" pad="14"/>
<connect gate="1" pin="CLR" pad="15"/>
<connect gate="1" pin="CO" pad="12"/>
<connect gate="1" pin="XCAP" pad="6"/>
<connect gate="1" pin="Y0" pad="2"/>
<connect gate="1" pin="Y1" pad="1"/>
<connect gate="1" pin="Y2" pad="3"/>
<connect gate="1" pin="Y3" pad="7"/>
<connect gate="1" pin="Y4" pad="11"/>
<connect gate="1" pin="Y5" pad="4"/>
<connect gate="1" pin="Y6" pad="5"/>
<connect gate="1" pin="Y7" pad="10"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7032" prefix="V">
<description>Quad 2-input &lt;b&gt;OR&lt;/b&gt;, schmitt trigger</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7032"/>
<gate name="/2" symbol="7032"/>
<gate name="/3" symbol="7032"/>
<gate name="/4" symbol="7032"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="9"/>
<connect gate="/3" pin="B" pad="10"/>
<connect gate="/3" pin="Y" pad="8"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7074" prefix="V">
<description>Dual J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, &lt;b&gt;INVERTER/NOR/NAND&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7074_6"/>
<gate name="/2" symbol="7074_5"/>
<gate name="/3" symbol="7074_4"/>
<gate name="/4" symbol="7074_3"/>
<gate name="/5" symbol="7074_2"/>
<gate name="/6" symbol="7074_1"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="/1" pin="A" pad="20"/>
<connect gate="/1" pin="B" pad="21"/>
<connect gate="/1" pin="Y" pad="19"/>
<connect gate="/2" pin="!CLR" pad="14"/>
<connect gate="/2" pin="!PRE" pad="17"/>
<connect gate="/2" pin="!Q" pad="15"/>
<connect gate="/2" pin="CLK" pad="18"/>
<connect gate="/2" pin="D" pad="16"/>
<connect gate="/2" pin="Q" pad="13"/>
<connect gate="/3" pin="!CLR" pad="10"/>
<connect gate="/3" pin="!PRE" pad="7"/>
<connect gate="/3" pin="!Q" pad="9"/>
<connect gate="/3" pin="CLK" pad="6"/>
<connect gate="/3" pin="D" pad="8"/>
<connect gate="/3" pin="Q" pad="11"/>
<connect gate="/4" pin="A" pad="3"/>
<connect gate="/4" pin="B" pad="4"/>
<connect gate="/4" pin="Y" pad="5"/>
<connect gate="/5" pin="A" pad="22"/>
<connect gate="/5" pin="Y" pad="2"/>
<connect gate="/6" pin="A" pad="1"/>
<connect gate="/6" pin="Y" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7075" prefix="V">
<description>J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, &lt;b&gt;INVERTER/NAND&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7075_6"/>
<gate name="/2" symbol="7075_5"/>
<gate name="/3" symbol="7075_4"/>
<gate name="/4" symbol="7075_3"/>
<gate name="/5" symbol="7075_2"/>
<gate name="/6" symbol="7075_1"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="/1" pin="A" pad="20"/>
<connect gate="/1" pin="B" pad="21"/>
<connect gate="/1" pin="Y" pad="19"/>
<connect gate="/2" pin="!CLR" pad="14"/>
<connect gate="/2" pin="!PRE" pad="17"/>
<connect gate="/2" pin="!Q" pad="15"/>
<connect gate="/2" pin="CLK" pad="18"/>
<connect gate="/2" pin="D" pad="16"/>
<connect gate="/2" pin="Q" pad="13"/>
<connect gate="/3" pin="!CLR" pad="10"/>
<connect gate="/3" pin="!PRE" pad="7"/>
<connect gate="/3" pin="!Q" pad="9"/>
<connect gate="/3" pin="CLK" pad="6"/>
<connect gate="/3" pin="D" pad="8"/>
<connect gate="/3" pin="Q" pad="11"/>
<connect gate="/4" pin="A" pad="3"/>
<connect gate="/4" pin="B" pad="4"/>
<connect gate="/4" pin="Y" pad="5"/>
<connect gate="/5" pin="A" pad="22"/>
<connect gate="/5" pin="Y" pad="2"/>
<connect gate="/6" pin="A" pad="1"/>
<connect gate="/6" pin="Y" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7076" prefix="V">
<description>J-K &lt;b&gt;FLIP FLOP&lt;/b&gt;, &lt;b&gt;INVERTER/NOR&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7076_6"/>
<gate name="/2" symbol="7076_5"/>
<gate name="/3" symbol="7076_4"/>
<gate name="/4" symbol="7076_3"/>
<gate name="/5" symbol="7076_2"/>
<gate name="/6" symbol="7076_1"/>
</gates>
<devices>
<device name="N" package="DIL24-3">
<connects>
<connect gate="/+UB" pin="+UB" pad="24"/>
<connect gate="/-UB" pin="-UB" pad="12"/>
<connect gate="/1" pin="A" pad="20"/>
<connect gate="/1" pin="B" pad="21"/>
<connect gate="/1" pin="Y" pad="19"/>
<connect gate="/2" pin="!CLR" pad="14"/>
<connect gate="/2" pin="!PRE" pad="17"/>
<connect gate="/2" pin="!Q" pad="15"/>
<connect gate="/2" pin="CLK" pad="18"/>
<connect gate="/2" pin="D" pad="16"/>
<connect gate="/2" pin="Q" pad="13"/>
<connect gate="/3" pin="!CLR" pad="10"/>
<connect gate="/3" pin="!PRE" pad="7"/>
<connect gate="/3" pin="!Q" pad="9"/>
<connect gate="/3" pin="CLK" pad="6"/>
<connect gate="/3" pin="D" pad="8"/>
<connect gate="/3" pin="Q" pad="11"/>
<connect gate="/4" pin="A" pad="3"/>
<connect gate="/4" pin="B" pad="4"/>
<connect gate="/4" pin="Y" pad="5"/>
<connect gate="/5" pin="A" pad="22"/>
<connect gate="/5" pin="Y" pad="2"/>
<connect gate="/6" pin="A" pad="1"/>
<connect gate="/6" pin="Y" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*7266" prefix="V">
<description>Quad 2-input &lt;b&gt;XNOR&lt;/b&gt;</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="7266"/>
<gate name="/2" symbol="7266"/>
<gate name="/3" symbol="7266"/>
<gate name="/4" symbol="7266"/>
</gates>
<devices>
<device name="N" package="DIL14">
<connects>
<connect gate="/+UB" pin="+UB" pad="14"/>
<connect gate="/-UB" pin="-UB" pad="7"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="5"/>
<connect gate="/2" pin="B" pad="6"/>
<connect gate="/2" pin="Y" pad="4"/>
<connect gate="/3" pin="A" pad="8"/>
<connect gate="/3" pin="B" pad="9"/>
<connect gate="/3" pin="Y" pad="10"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*804" prefix="V">
<description>Hex &lt;b&gt;NAND&lt;/b&gt; driver</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="804"/>
<gate name="/2" symbol="804"/>
<gate name="/3" symbol="804"/>
<gate name="/4" symbol="804"/>
<gate name="/5" symbol="804"/>
<gate name="/6" symbol="804"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="7"/>
<connect gate="/3" pin="B" pad="8"/>
<connect gate="/3" pin="Y" pad="9"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
<connect gate="/5" pin="A" pad="15"/>
<connect gate="/5" pin="B" pad="16"/>
<connect gate="/5" pin="Y" pad="14"/>
<connect gate="/6" pin="A" pad="18"/>
<connect gate="/6" pin="B" pad="19"/>
<connect gate="/6" pin="Y" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*805" prefix="V">
<description>Hex &lt;b&gt;NOR&lt;/b&gt; driver</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="805"/>
<gate name="/2" symbol="805"/>
<gate name="/3" symbol="805"/>
<gate name="/4" symbol="805"/>
<gate name="/5" symbol="805"/>
<gate name="/6" symbol="805"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="7"/>
<connect gate="/3" pin="B" pad="8"/>
<connect gate="/3" pin="Y" pad="9"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
<connect gate="/5" pin="A" pad="15"/>
<connect gate="/5" pin="B" pad="16"/>
<connect gate="/5" pin="Y" pad="14"/>
<connect gate="/6" pin="A" pad="18"/>
<connect gate="/6" pin="B" pad="19"/>
<connect gate="/6" pin="Y" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*808" prefix="V">
<description>Hex &lt;b&gt;AND&lt;/b&gt; driver</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="808"/>
<gate name="/2" symbol="808"/>
<gate name="/3" symbol="808"/>
<gate name="/4" symbol="808"/>
<gate name="/5" symbol="808"/>
<gate name="/6" symbol="808"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="7"/>
<connect gate="/3" pin="B" pad="8"/>
<connect gate="/3" pin="Y" pad="9"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
<connect gate="/5" pin="A" pad="15"/>
<connect gate="/5" pin="B" pad="16"/>
<connect gate="/5" pin="Y" pad="14"/>
<connect gate="/6" pin="A" pad="18"/>
<connect gate="/6" pin="B" pad="19"/>
<connect gate="/6" pin="Y" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*832" prefix="V">
<description>Hex &lt;b&gt;OR&lt;/b&gt; driver</description>
<gates>
<gate name="/+UB" symbol="+UB"/>
<gate name="/-UB" symbol="-UB"/>
<gate name="/1" symbol="832"/>
<gate name="/2" symbol="832"/>
<gate name="/3" symbol="832"/>
<gate name="/4" symbol="832"/>
<gate name="/5" symbol="832"/>
<gate name="/6" symbol="832"/>
</gates>
<devices>
<device name="N" package="DIL20">
<connects>
<connect gate="/+UB" pin="+UB" pad="20"/>
<connect gate="/-UB" pin="-UB" pad="10"/>
<connect gate="/1" pin="A" pad="1"/>
<connect gate="/1" pin="B" pad="2"/>
<connect gate="/1" pin="Y" pad="3"/>
<connect gate="/2" pin="A" pad="4"/>
<connect gate="/2" pin="B" pad="5"/>
<connect gate="/2" pin="Y" pad="6"/>
<connect gate="/3" pin="A" pad="7"/>
<connect gate="/3" pin="B" pad="8"/>
<connect gate="/3" pin="Y" pad="9"/>
<connect gate="/4" pin="A" pad="12"/>
<connect gate="/4" pin="B" pad="13"/>
<connect gate="/4" pin="Y" pad="11"/>
<connect gate="/5" pin="A" pad="15"/>
<connect gate="/5" pin="B" pad="16"/>
<connect gate="/5" pin="Y" pad="14"/>
<connect gate="/6" pin="A" pad="18"/>
<connect gate="/6" pin="B" pad="19"/>
<connect gate="/6" pin="Y" pad="17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P+UB" prefix="IC">
<description>Supply +UB</description>
<gates>
<gate name="G$1" symbol="+UB"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="P-UB" prefix="IC">
<description>Supply -UB</description>
<gates>
<gate name="G$1" symbol="-UB"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*4053" prefix="V">
<description>&lt;b&gt;Triple 2-channel analog multiplexer/demultiplexer&lt;/b&gt;&lt;p&gt;
Philips Semiconductor</description>
<gates>
<gate name="G$1" symbol="4053"/>
<gate name="P1" symbol="PWRVCCGNDVEE"/>
</gates>
<devices>
<device name="P" package="DIL16">
<connects>
<connect gate="G$1" pin="!G" pad="6"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="P1" pin="GND" pad="8"/>
<connect gate="P1" pin="VCC" pad="16"/>
<connect gate="P1" pin="VEE" pad="7"/>
</connects>
<technologies>
<technology name="HC"/>
<technology name="HCT"/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
