<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.2">
<drawing>
<library>
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
SOT753 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
<package name="SC70-5">
<description>&lt;b&gt;SMT SC70-5&lt;/b&gt;&lt;p&gt;
SOT353 - Philips Semiconductors&lt;br&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
</package>
<package name="SSOP08">
<description>&lt;b&gt;SMT SSOP 08&lt;/b&gt;</description>
</package>
<package name="MAC06A">
<description>&lt;b&gt;6-Lead MicroPak, 1.0mm Wide&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/ds/NC/NC7SZ14.pdf</description>
</package>
<package name="DBV_R-PDSO-G6">
<description>&lt;b&gt;DBV (R-PDSO-G6)&lt;/b&gt; PLASTIC SMALL-OUTLINE PACKAGE&lt;p&gt;
SOT (SOT-23) - DBV&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g3157.</description>
</package>
<package name="DCK_R-PDSO-G6">
<description>&lt;b&gt;DCK (R-PDSO-G6)&lt;/b&gt; PLASTIC SMALL-OUTLINE PACKAGE&lt;p&gt;
SOT (SC-70) - DCK&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g3157.</description>
</package>
<package name="DRL_R-PDSO-N6">
<description>&lt;b&gt;DRL (R-PDSO-N6)&lt;/b&gt; PLASTIC SMALL OUTLINE&lt;p&gt;
SOT (SOT-553) -  DRL&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g3157.pdf</description>
</package>
<package name="YZP_R-XBGA-N6">
<description>&lt;b&gt;YZP (R-XBGA-N6)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
NanoFree TM -  WCSP (DSBGA) 0.23-mm Large Bump - YZP (Pb-free)&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g3157</description>
</package>
<package name="YEP_R-XBGA-N6">
<description>&lt;b&gt;YEP (R-XBGA-N6)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
NanoStar TM - WCSP (DSBG A)0.23-mm Large Bump - YEP&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g3157</description>
</package>
<package name="DRL_R-PDSO-N5">
<description>&lt;b&gt;DRL (R-PDSO-N5)&lt;/b&gt; PLASTIC SMALL OUTLINE&lt;p&gt;
SOT (SOT-553) -  DRL&lt;br&gt;
http://focus.ti.com/lit/ds/symlink/sn74lvc1g66.pdf</description>
</package>
<package name="DCK_R-PDSO-G5">
<description>&lt;b&gt;DCK (R-PDSO-G5)&lt;/b&gt; PLASTIC SMALL-OUTLINE PACKAGE&lt;p&gt;
SOT (SC-70) - DCK&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g66.pdf</description>
</package>
<package name="DBV_R-PDSO-G5">
<description>&lt;b&gt;DBV (R-PDSO-G5)&lt;/b&gt; PLASTIC SMALL-OUTLINE PACKAGE&lt;p&gt;
SOT (SOT-23) - DBV&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g66.pdf</description>
</package>
<package name="YEP_R-XBGA-N5">
<description>&lt;b&gt;YEP (R-XBGA-N5)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
NanoStar TM - WCSP (DSBG A)0.23-mm Large Bump - YEP&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g66.pdf</description>
</package>
<package name="YZP_R-XBGA-N5">
<description>&lt;b&gt;YZP (R-XBGA-N5)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
NanoFree TM -  WCSP (DSBGA) 0.23-mm Large Bump - YZP (Pb-free)&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g66.pdf</description>
</package>
<package name="YEA_R-XBGA-N5">
<description>&lt;b&gt;YEA (R-XBGA-N5)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
NanoStar TM - WCSP (DSBG A)0.23-mm Large Bump - YEA&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g66.pdf</description>
</package>
<package name="YZA_R-XBGA-N5">
<description>&lt;b&gt;YZA (R-XBGA-N5)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
NanoStar TM - WCSP (DSBG A)0.23-mm Large Bump - YZA&lt;br&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g66.pdf</description>
</package>
<package name="DCT_R-PDSO-G8">
<description>&lt;b&gt;DCT (R-PDSO-G8)&lt;/b&gt; PLSTIG SMALL-OUTLINE PACKAGE&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc2g53.pdf</description>
</package>
<package name="DCU_R-PDSO-G8">
<description>&lt;b&gt;DCU (R-PDSO-G8)&lt;/b&gt; PLASTIC SMALL-OUTLINE PACKAGE (DIE DOWN)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc2g53.pdf</description>
</package>
<package name="YEA_R-XBGA-N8">
<description>&lt;b&gt;YEA (R-XBGA-N8)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc2g53.pdf</description>
</package>
<package name="YZA_R-XBGA-N8">
<description>&lt;b&gt;YZA (R-XBGA-N8)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc2g53.pdf</description>
</package>
<package name="YZP_R-XBGA-N8">
<description>&lt;b&gt;YZP (R-XBGA-N8)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc2g53.pdf</description>
</package>
<package name="YEP_R-XBGA-N8">
<description>&lt;b&gt;YEP (R-XBGA-N8)&lt;/b&gt; DIE-SIZE BALL GRID ARRAY&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc2g53.pdf</description>
</package>
</packages>
<symbols>
<symbol name="7404">
<pin name="I" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7405">
<pin name="I" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="7407">
<pin name="I" direction="in"/>
<pin name="O" direction="oc"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="74125">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="hiz"/>
</symbol>
<symbol name="74126">
<pin name="OE" direction="in"/>
<pin name="I" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7400">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7401">
<pin name="O" direction="oc" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7402">
<pin name="O" direction="out" function="dot"/>
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
</symbol>
<symbol name="7403">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="oc" function="dot"/>
</symbol>
<symbol name="7408">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7432">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7486">
<pin name="I0" direction="in"/>
<pin name="I1" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7414">
<pin name="I" direction="in"/>
<pin name="O" direction="out" function="dot"/>
</symbol>
<symbol name="7417">
<pin name="I" direction="in"/>
<pin name="O" direction="out"/>
</symbol>
<symbol name="7466">
<pin name="E" direction="in"/>
<pin name="Y"/>
<pin name="Z"/>
</symbol>
<symbol name="743157">
<pin name="!A!/B" direction="in"/>
<pin name="A"/>
<pin name="B"/>
<pin name="X"/>
</symbol>
<symbol name="7453">
<pin name="A" direction="in"/>
<pin name="Y1"/>
<pin name="Y2"/>
<pin name="COM"/>
<pin name="INH" direction="in"/>
</symbol>
<symbol name="PWRN2">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
</symbol>
<symbol name="7479">
<pin name="D" direction="in"/>
<pin name="C" direction="in"/>
<pin name="Q" direction="out"/>
</symbol>
<symbol name="7479-1">
<pin name="D" direction="in"/>
<pin name="CLK" direction="in" function="clk"/>
<pin name="Q" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="74*1G04" prefix="IC">
<description>&lt;b&gt;INVERTER&lt;/b&gt; Gate</description>
<gates>
<gate name="A" symbol="7404"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G07" prefix="IC">
<description>Single &lt;b&gt;Buffer/Driver&lt;/b&gt; With Open-Drain Output</description>
<gates>
<gate name="A" symbol="7407"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G00" prefix="IC">
<description>2-input &lt;b&gt;NAND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7400"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G02" prefix="IC">
<description>2-input &lt;b&gt;NOR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7402"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G08" prefix="IC">
<description>2-input &lt;b&gt;AND&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7408"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G32" prefix="IC">
<description>2-input &lt;b&gt;OR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7432"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G86" prefix="IC">
<description>2-input &lt;b&gt;EXCLUSIV-OR&lt;/b&gt; gate</description>
<gates>
<gate name="A" symbol="7486"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I0" pad="1"/>
<connect gate="A" pin="I1" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G125" prefix="IC">
<description>Single Bus &lt;b&gt;Buffer &lt;/b&gt;Gate with 3-State Output</description>
<gates>
<gate name="A" symbol="74125"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="CBT"/>
<technology name="CBTLV"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="CBT"/>
<technology name="CBTLV"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G126" prefix="IC">
<description>Single Bus &lt;b&gt;Buffer&lt;/b&gt; Gate With 3-State Outputs</description>
<gates>
<gate name="A" symbol="74126"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G14" prefix="IC">
<description>Single &lt;b&gt;Schmitt-Trigger Inverter &lt;/b&gt;Gate</description>
<gates>
<gate name="A" symbol="7414"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
<technology name="AHCT"/>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1GU04" prefix="IC">
<description>Single Unbuffered Inverter</description>
<gates>
<gate name="G$1" symbol="7404"/>
<gate name="G$2" symbol="PWRN"/>
</gates>
<devices>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="G$2" pin="GND" pad="3"/>
<connect gate="G$2" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="G$2" pin="GND" pad="3"/>
<connect gate="G$2" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AHC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*2G125" prefix="IC">
<description>Dual line drivers with 3-state outputs.</description>
<gates>
<gate name="G$1" symbol="74125"/>
<gate name="G$2" symbol="74125"/>
<gate name="G$3" symbol="PWRN"/>
</gates>
<devices>
<device name="DCT" package="SSOP08">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="6"/>
<connect gate="G$1" pin="OE" pad="1"/>
<connect gate="G$2" pin="I" pad="5"/>
<connect gate="G$2" pin="O" pad="3"/>
<connect gate="G$2" pin="OE" pad="7"/>
<connect gate="G$3" pin="GND" pad="4"/>
<connect gate="G$3" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G06" prefix="IC">
<description>Single Inverter Buffer/Driver With Open-Drain Output</description>
<gates>
<gate name="G$1" symbol="7405"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G17" prefix="IC">
<description>Single Schmitt-Trigger Buffer</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G$1" symbol="7417"/>
</gates>
<devices>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="AUC"/>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G240" prefix="IC">
<description>Single Buffer/Driver With 3-State Outputs</description>
<gates>
<gate name="G$1" symbol="74125"/>
<gate name="G$2" symbol="PWRN"/>
</gates>
<devices>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="G$1" pin="OE" pad="1"/>
<connect gate="G$2" pin="GND" pad="3"/>
<connect gate="G$2" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="G$1" pin="OE" pad="1"/>
<connect gate="G$2" pin="GND" pad="3"/>
<connect gate="G$2" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G66" prefix="IC">
<description>&lt;b&gt;Single Analog / Bilateral Switch&lt;/b&gt;&lt;p&gt;
Source: http://www.semiconductors.philips.com/acrobat_download/datasheets/74HC_HCT1G66_3.pdf</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G$2" symbol="7466"/>
</gates>
<devices>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="G$2" pin="E" pad="4"/>
<connect gate="G$2" pin="Y" pad="1"/>
<connect gate="G$2" pin="Z" pad="2"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$2" pin="E" pad="4"/>
<connect gate="G$2" pin="Y" pad="1"/>
<connect gate="G$2" pin="Z" pad="2"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DRL" package="DRL_R-PDSO-N6">
<connects>
<connect gate="G$2" pin="E" pad="4"/>
<connect gate="G$2" pin="Y" pad="1"/>
<connect gate="G$2" pin="Z" pad="2"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="YEA" package="YEA_R-XBGA-N5">
<connects>
<connect gate="G$2" pin="E" pad="C2"/>
<connect gate="G$2" pin="Y" pad="A1"/>
<connect gate="G$2" pin="Z" pad="B1"/>
<connect gate="P" pin="GND" pad="C1"/>
<connect gate="P" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="YEP" package="YEP_R-XBGA-N5">
<connects>
<connect gate="G$2" pin="E" pad="C2"/>
<connect gate="G$2" pin="Y" pad="A1"/>
<connect gate="G$2" pin="Z" pad="B1"/>
<connect gate="P" pin="GND" pad="C1"/>
<connect gate="P" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="YZA" package="YZA_R-XBGA-N5">
<connects>
<connect gate="G$2" pin="E" pad="C2"/>
<connect gate="G$2" pin="Y" pad="A1"/>
<connect gate="G$2" pin="Z" pad="B1"/>
<connect gate="P" pin="GND" pad="C1"/>
<connect gate="P" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DCT" package="DCT_R-PDSO-G8">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G79" prefix="IC">
<description>Single Positive-Edge-Triggered D-Type Flip-Flop&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/sn74lvc1g79.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G$1" symbol="7479"/>
</gates>
<devices>
<device name="DCK" package="SC70-5">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="Q" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LVC"/>
</technologies>
</device>
<device name="DBV" package="SOT23-5">
<connects>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="D" pad="1"/>
<connect gate="G$1" pin="Q" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name="LVC"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC7SZ14" prefix="IC">
<description>&lt;b&gt;TinyLogic(R) UHS Inverter with Schmitt Trigger Input&lt;/b&gt;&lt;p&gt;
Source: http://www.fairchildsemi.com/ds/NC/NC7SZ14.pdf</description>
<gates>
<gate name="G$1" symbol="7414"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="M5X" package="SOT23-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="P5X" package="SC70-5">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="L6X" package="MAC06A">
<connects>
<connect gate="G$1" pin="I" pad="2"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="VCC" pad="6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G3157" prefix="IC">
<description>&lt;b&gt;Single-Pole, Double-Throw Analog Switch&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc1g3157.pdf</description>
<gates>
<gate name="G$1" symbol="743157"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="ZYPR" package="YZP_R-XBGA-N6">
<connects>
<connect gate="G$1" pin="!A!/B" pad="A2"/>
<connect gate="G$1" pin="A" pad="C1"/>
<connect gate="G$1" pin="B" pad="A1"/>
<connect gate="G$1" pin="X" pad="C2"/>
<connect gate="P" pin="GND" pad="B1"/>
<connect gate="P" pin="VCC" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DBVR" package="DBV_R-PDSO-G6">
<connects>
<connect gate="G$1" pin="!A!/B" pad="6"/>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="X" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DCKR" package="DCK_R-PDSO-G6">
<connects>
<connect gate="G$1" pin="!A!/B" pad="6"/>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="X" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DRLR" package="DRL_R-PDSO-N6">
<connects>
<connect gate="G$1" pin="!A!/B" pad="6"/>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="1"/>
<connect gate="G$1" pin="X" pad="4"/>
<connect gate="P" pin="GND" pad="2"/>
<connect gate="P" pin="VCC" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="YEPR" package="YEP_R-XBGA-N6">
<connects>
<connect gate="G$1" pin="!A!/B" pad="A2"/>
<connect gate="G$1" pin="A" pad="C1"/>
<connect gate="G$1" pin="B" pad="A1"/>
<connect gate="G$1" pin="X" pad="C2"/>
<connect gate="P" pin="GND" pad="B1"/>
<connect gate="P" pin="VCC" pad="B2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*1G53" prefix="IC">
<description>&lt;b&gt;SINGLE-POLE DOUBLE-THROW (SPDT) ANALOG SWITCH&lt;/b&gt; 2:1 ANALOG MULTIPLEXER/DEMULTIPLEXER&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc2g53.pdf</description>
<gates>
<gate name="G$1" symbol="7453"/>
<gate name="P" symbol="PWRN2"/>
</gates>
<devices>
<device name="DCT" package="DCT_R-PDSO-G8">
<connects>
<connect gate="G$1" pin="A" pad="5"/>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="INH" pad="2"/>
<connect gate="G$1" pin="Y1" pad="7"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DCU" package="DCU_R-PDSO-G8">
<connects>
<connect gate="G$1" pin="A" pad="5"/>
<connect gate="G$1" pin="COM" pad="1"/>
<connect gate="G$1" pin="INH" pad="2"/>
<connect gate="G$1" pin="Y1" pad="7"/>
<connect gate="G$1" pin="Y2" pad="6"/>
<connect gate="P" pin="GND" pad="3"/>
<connect gate="P" pin="GND@1" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="YEA" package="YEA_R-XBGA-N8">
<connects>
<connect gate="G$1" pin="A" pad="D2"/>
<connect gate="G$1" pin="COM" pad="A1"/>
<connect gate="G$1" pin="INH" pad="B1"/>
<connect gate="G$1" pin="Y1" pad="B2"/>
<connect gate="G$1" pin="Y2" pad="C2"/>
<connect gate="P" pin="GND" pad="C1"/>
<connect gate="P" pin="GND@1" pad="D1"/>
<connect gate="P" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="YEP" package="YEP_R-XBGA-N8">
<connects>
<connect gate="G$1" pin="A" pad="D2"/>
<connect gate="G$1" pin="COM" pad="A1"/>
<connect gate="G$1" pin="INH" pad="B1"/>
<connect gate="G$1" pin="Y1" pad="B2"/>
<connect gate="G$1" pin="Y2" pad="C2"/>
<connect gate="P" pin="GND" pad="C1"/>
<connect gate="P" pin="GND@1" pad="D1"/>
<connect gate="P" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="YZA" package="YZA_R-XBGA-N8">
<connects>
<connect gate="G$1" pin="A" pad="D2"/>
<connect gate="G$1" pin="COM" pad="A1"/>
<connect gate="G$1" pin="INH" pad="B1"/>
<connect gate="G$1" pin="Y1" pad="B2"/>
<connect gate="G$1" pin="Y2" pad="C2"/>
<connect gate="P" pin="GND" pad="C1"/>
<connect gate="P" pin="GND@1" pad="D1"/>
<connect gate="P" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN74LVC2G126" prefix="IC">
<description>&lt;b&gt;Dual Bus Buffer Gate With 3-State Outputs&lt;/b&gt;&lt;p&gt;
Source: http://www.ti.com.cn/cn/lit/ds/symlink/sn74lvc2g126.pdf</description>
<gates>
<gate name="A" symbol="74126"/>
<gate name="B" symbol="74126"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="DCT" package="DCT_R-PDSO-G8">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="B" pin="OE" pad="7"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DCU" package="DCU_R-PDSO-G8">
<connects>
<connect gate="A" pin="I" pad="2"/>
<connect gate="A" pin="O" pad="6"/>
<connect gate="A" pin="OE" pad="1"/>
<connect gate="B" pin="I" pad="5"/>
<connect gate="B" pin="O" pad="3"/>
<connect gate="B" pin="OE" pad="7"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="74*2G79" prefix="IC">
<description>&lt;b&gt;Single Positive-Edge-Triggered D-Type Flip-Flop&lt;/b&gt;&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/sn74lvc2g79.pdf</description>
<gates>
<gate name="A" symbol="7479-1"/>
<gate name="P" symbol="PWRN"/>
<gate name="B" symbol="7479-1"/>
</gates>
<devices>
<device name="DCT" package="DCT_R-PDSO-G8">
<connects>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="B" pin="CLK" pad="5"/>
<connect gate="B" pin="D" pad="6"/>
<connect gate="B" pin="Q" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="DCU" package="DCU_R-PDSO-G8">
<connects>
<connect gate="A" pin="CLK" pad="1"/>
<connect gate="A" pin="D" pad="2"/>
<connect gate="A" pin="Q" pad="7"/>
<connect gate="B" pin="CLK" pad="5"/>
<connect gate="B" pin="D" pad="6"/>
<connect gate="B" pin="Q" pad="3"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="YEP" package="YEP_R-XBGA-N8">
<connects>
<connect gate="A" pin="CLK" pad="A1"/>
<connect gate="A" pin="D" pad="B1"/>
<connect gate="A" pin="Q" pad="B2"/>
<connect gate="B" pin="CLK" pad="D2"/>
<connect gate="B" pin="D" pad="C2"/>
<connect gate="B" pin="Q" pad="C1"/>
<connect gate="P" pin="GND" pad="D1"/>
<connect gate="P" pin="VCC" pad="A2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
