<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<library>
<description>&lt;b&gt;Crystals and Oscillators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by IQD Frequency Products&lt;/author&gt;</description>
<packages>
<package name="WATCH-3X8">
<description>&lt;b&gt;IQD Frequency Products SIL Package&lt;/b&gt;</description>
</package>
<package name="HC49">
<description>&lt;b&gt;IQD Frequency Products SIL Package&lt;/b&gt;</description>
</package>
<package name="HC49-4-HSMX">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="86SMX">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="3.4X2.7-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="5.2X3.4-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="7.5X5-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="3.2X1.5-2-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="HC49-3L">
<description>&lt;b&gt;IQD Frequency Products SIL Package&lt;/b&gt;</description>
</package>
<package name="7.5X5-2-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="85SMX">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="90SMX">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="91SMX">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="2.5X2-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="2.6X2.1-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="2.0X1.2-2PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="2.0X1.6-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="7.2X5.2-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="5.0X3.2-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="7.0X5.0-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="5.0X3.2-TCXO">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="7.0X5.0-10-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
<package name="CO-15-1">
<description>&lt;b&gt;IQD Frequency Products Package&lt;/b&gt;</description>
</package>
<package name="CO-08-5">
<description>&lt;b&gt;IQD Frequency Products Package&lt;/b&gt;</description>
</package>
<package name="CS-09-9">
<description>&lt;b&gt;IQD Frequency Products Package&lt;/b&gt;</description>
</package>
<package name="C0-08-8">
<description>&lt;b&gt;IQD Frequency Products Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="CRYSTAL">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="OSC">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="OSC-WITH-OE">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="FO" direction="out"/>
<pin name="OE" direction="in"/>
</symbol>
<symbol name="QG2">
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="CON" direction="in"/>
</symbol>
<symbol name="OSC-WITH-TS">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="TS" direction="pas"/>
</symbol>
<symbol name="CRYSTAL-WITH-GND">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="OSC-NO-OE">
<pin name="GND" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="TRI" direction="in"/>
</symbol>
<symbol name="Q-SHIELD2">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="TCXO">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="VC" direction="in"/>
</symbol>
<symbol name="TCXO-6-PIN">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="TS-E" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="VC" direction="in"/>
</symbol>
<symbol name="TCXO-OE-ONLY">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="TS" direction="in"/>
</symbol>
<symbol name="OCXO">
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="OUT" direction="out"/>
<pin name="VC" direction="in"/>
<pin name="VREF" direction="out"/>
</symbol>
<symbol name="6-PIN-OCXO">
<description>6 PIN OCXO</description>
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="GND" direction="pwr"/>
<pin name="ALM" direction="out"/>
<pin name="VC" direction="in"/>
</symbol>
<symbol name="SMD-OCXO">
<pin name="VCC" direction="pwr"/>
<pin name="VREF" direction="out"/>
<pin name="OUT" direction="out"/>
<pin name="VC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="ALM" direction="out"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CRYSTALS-NOGND" prefix="X">
<description>&lt;b&gt;CRYSTALS CAN NOT GROUNDED&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CRYSTAL"/>
</gates>
<devices>
<device name="-HC49" package="HC49">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-4-HSMX" package="HC49-4-HSMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-WATCH-3X8" package="WATCH-3X8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-86SMX" package="86SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-85SMX" package="85SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-90SMX" package="90SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-91SMX" package="91SMX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-12SMX-A" package="7.5X5-2-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-12SMX-B" package="7.5X5-4-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPX-217" package="3.2X1.5-2-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQXC-25" package="2.0X1.2-2PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-HC49/4H" package="HC49">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OSC-OE" prefix="OS">
<description>&lt;b&gt;OSCILLATOR WITH OE&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="QG2"/>
</gates>
<devices>
<device name="-CFPS-107" package="2.6X2.1-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPS-108" package="2.6X2.1-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPS-109" package="2.6X2.1-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPS-32" package="7.2X5.2-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPS-39" package="3.4X2.7-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPS-69" package="5.0X3.2-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPS-72" package="7.2X5.2-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPS-73" package="7.2X5.2-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPS-9" package="5.2X3.4-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQXO-540" package="2.0X1.6-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQXO-541" package="2.0X1.6-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQXO-542" package="2.0X1.6-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQXO-793" package="2.5X2-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQXO-794" package="2.5X2-4-PAD">
<connects>
<connect gate="A" pin="CON" pad="1"/>
<connect gate="A" pin="OUT" pad="3"/>
<connect gate="A" pin="VDD" pad="4"/>
<connect gate="A" pin="VSS" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HC49" prefix="X">
<description>&lt;b&gt;Crystals&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CRYSTAL-WITH-GND"/>
</gates>
<devices>
<device name="-HC49-3L" package="HC49-3L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MFD" value="IQD Frequency Products"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CRYSTALS-GND-LID" prefix="X">
<description>&lt;b&gt;CRYSTALS WITH CAN GROUNDED&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="Q-SHIELD2"/>
</gates>
<devices>
<device name="-4-PAD" package="7.5X5-4-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="12SMX-B"/>
</technologies>
</device>
<device name="-CFPX-104" package="5.2X3.4-4-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPX-180" package="3.4X2.7-4-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPX-181" package="2.5X2-4-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPX-218" package="2.6X2.1-4-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQXC-42" package="2.0X1.6-4-PAD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCXO" prefix="TC">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TCXO"/>
</gates>
<devices>
<device name="-CFPT-125" package="7.0X5.0-4-PAD">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPT-126" package="7.0X5.0-4-PAD">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CFPT-9301" package="5.0X3.2-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TCXO-NO-VC" prefix="TC">
<description>&lt;b&gt;CRYSTAL RESONATOR&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OSC"/>
</gates>
<devices>
<device name="-CFPT-127" package="5.0X3.2-TCXO">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="VCC" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CFPT-9006" prefix="TC">
<description>&lt;b&gt;Temperature Compensated Xtal Oscillator&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TCXO-6-PIN"/>
</gates>
<devices>
<device name="-CFPT-9006" package="7.0X5.0-10-PAD">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="TS-E" pad="8"/>
<connect gate="G$1" pin="VC" pad="10"/>
<connect gate="G$1" pin="VCC" pad="9"/>
<connect gate="G$1" pin="VREF" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MFD" value="IQD Frequency Products"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="E2747" prefix="X">
<description>&lt;b&gt;Temperature Compensated Xtal Oscillator&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TCXO-OE-ONLY"/>
</gates>
<devices>
<device name="-E2747" package="7.0X5.0-10-PAD">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="OUT" pad="5"/>
<connect gate="G$1" pin="TS" pad="8"/>
<connect gate="G$1" pin="VCC" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MFD" value="IQD Frequency Products"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OCXO" prefix="XO">
<description>&lt;b&gt;Oven controlled Xtal Oscillator&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="OCXO"/>
</gates>
<devices>
<device name="-IQOV-50-6" package="CO-15-1">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VC" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-50-7" package="CO-15-1">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VC" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-50-8" package="CO-15-1">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VC" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-50-9" package="CO-15-1">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VC" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-50-10" package="CO-15-1">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VC" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-50-11" package="CO-15-1">
<connects>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="OUT" pad="2"/>
<connect gate="G$1" pin="VC" pad="4"/>
<connect gate="G$1" pin="VCC" pad="1"/>
<connect gate="G$1" pin="VREF" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-70-6" package="C0-08-8">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-70-9" package="C0-08-8">
<connects>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OCXO-6-PIN" prefix="XO">
<description>&lt;b&gt;Oven controlled Xtal Oscillator&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="6-PIN-OCXO"/>
</gates>
<devices>
<device name="-IQOV-70-7" package="CO-08-5">
<connects>
<connect gate="G$1" pin="ALM" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-70-8" package="CO-08-5">
<connects>
<connect gate="G$1" pin="ALM" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SMD-OCXO" prefix="XO">
<description>&lt;b&gt; SMD Oven Controlled Xtal Oscillator&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="SMD-OCXO"/>
</gates>
<devices>
<device name="-IQOV-90-18" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-19" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-20" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-21" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-22" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-23" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-24" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-25" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-26" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-27" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-28" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IQOV-90-29" package="CS-09-9">
<connects>
<connect gate="G$1" pin="ALM" pad="5"/>
<connect gate="G$1" pin="GND" pad="7"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VC" pad="1"/>
<connect gate="G$1" pin="VCC" pad="3"/>
<connect gate="G$1" pin="VREF" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
