<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Altera Programmable Logic Devices&lt;/b&gt;&lt;p&gt;
FLEX 10K&lt;p&gt;
MAX 7000&lt;p&gt;
MAX 9000&lt;p&gt;
FLEX 6000&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt; Databook, January 1998
&lt;li&gt;CD-ROM Gigital-Library, December 1998
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PQFP208">
<description>&lt;b&gt;Plastic Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="RQFP208">
<description>&lt;b&gt;Power Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PQFP160">
<description>&lt;b&gt;Plastic Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP100">
<description>Plastic &lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PQFP100">
<description>&lt;b&gt;Plastic Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="TQFP44">
<description>Plastic &lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PGA160">
<description>&lt;b&gt;Pin Grid Array&lt;/b&gt;</description>
</package>
<package name="PGA192">
<description>&lt;b&gt;Pin Grid Array&lt;/b&gt;</description>
</package>
<package name="PQFP240">
<description>&lt;b&gt;Plastic Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="RQFP240">
<description>&lt;b&gt;Power Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="PGA280">
<description>&lt;b&gt;Pin Grid Array&lt;/b&gt;</description>
</package>
<package name="RQFP304">
<description>&lt;b&gt;Power Quad Flat Pack&lt;/b&gt;</description>
</package>
<package name="BGA356">
<description>&lt;b&gt;Ball Grid Array&lt;/b&gt;</description>
</package>
<package name="PGA503">
<description>&lt;b&gt;Pin Grid Array&lt;/b&gt;</description>
</package>
<package name="PGA599">
<description>&lt;b&gt;Pin Grid Array&lt;/b&gt;</description>
</package>
<package name="BGA600">
<description>&lt;b&gt;Ball Grid Array&lt;/b&gt;</description>
</package>
<package name="PLCC84">
<description>&lt;b&gt;Plastic J-Lead Chip Carrier&lt;/b&gt;</description>
</package>
<package name="PLCC44">
<description>&lt;b&gt;Plastic J-Lead Chip Carrier&lt;/b&gt;</description>
</package>
<package name="PLCC68">
<description>&lt;b&gt;Plastic J-Lead Chip Carrier&lt;/b&gt;</description>
</package>
<package name="FBGA484">
<description>&lt;b&gt;Fine Ball Grid Array&lt;/b&gt;</description>
</package>
<package name="BGA672">
<description>&lt;b&gt;Ball Grid Array&lt;/b&gt;</description>
</package>
<package name="FBGA256">
<description>&lt;b&gt;Fine Ball Grid Array&lt;/b&gt;</description>
</package>
<package name="LOGO_10MM">
<description>&lt;b&gt;LOGO&lt;/b&gt;</description>
</package>
<package name="LOGO_20MM">
<description>&lt;b&gt;LOGO&lt;/b&gt;</description>
</package>
<package name="PLCC-S44">
<description>&lt;b&gt;Plastic Leaded Chip Carrier&lt;/b&gt; Socked</description>
</package>
<package name="FBGA100">
<description>&lt;b&gt;EPM240F100&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 36&lt;/i&gt;&lt;br&gt;
Source: EPM240F100.BSD</description>
</package>
<package name="MBGA100">
<description>&lt;b&gt;EPM240M100&lt;/b&gt; &lt;font color="red"&gt;edit this description&lt;/font&gt;&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 36&lt;/i&gt;&lt;br&gt;
Source: EPM240M100.BSD</description>
</package>
</packages>
<symbols>
<symbol name="EPM7064S">
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="IO8/TDI"/>
<pin name="IO9"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO31"/>
<pin name="IO32/TMS"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO39"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="TCK/IO48"/>
<pin name="IO49"/>
<pin name="IO50"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO55"/>
<pin name="TDO/IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
</symbol>
<symbol name="EPM7256">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO39"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO50"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO55"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO66"/>
<pin name="IO67"/>
<pin name="IO68"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO75"/>
<pin name="IO76"/>
<pin name="IO77"/>
<pin name="IO78"/>
<pin name="IO79"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO87"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO90"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO95"/>
<pin name="IO96"/>
<pin name="IO97"/>
<pin name="IO98"/>
<pin name="IO99"/>
<pin name="IO100"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO106"/>
<pin name="IO107"/>
<pin name="IO108"/>
<pin name="IO109"/>
<pin name="IO110"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO115"/>
<pin name="IO116"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO119"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
<pin name="IO125"/>
<pin name="IO126"/>
<pin name="IO127"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO130"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO135"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO138"/>
<pin name="IO139"/>
<pin name="IO140"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO146"/>
<pin name="IO147"/>
<pin name="IO148"/>
<pin name="IO149"/>
<pin name="IO150"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO155"/>
<pin name="IO156"/>
<pin name="IO157"/>
<pin name="IO158"/>
<pin name="IO159"/>
<pin name="IO160"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
<pin name="IO165"/>
<pin name="IO166"/>
<pin name="IO167"/>
<pin name="IO168"/>
<pin name="IO169"/>
<pin name="IO170"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO174"/>
<pin name="IO175"/>
<pin name="IO176"/>
<pin name="IO177"/>
<pin name="IO178"/>
<pin name="IO179"/>
<pin name="IO180"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO185"/>
<pin name="IO186"/>
<pin name="IO187"/>
<pin name="IO188"/>
<pin name="IO189"/>
<pin name="IO190"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO194"/>
<pin name="IO195"/>
<pin name="IO196"/>
<pin name="IO197"/>
<pin name="IO198"/>
<pin name="IO199"/>
<pin name="IO200"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO205"/>
<pin name="IO206"/>
<pin name="IO207"/>
<pin name="IO208"/>
<pin name="IO209"/>
<pin name="IO210"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO215"/>
<pin name="IO216"/>
<pin name="IO217"/>
<pin name="IO218"/>
<pin name="IO219"/>
<pin name="IO220"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO224"/>
<pin name="IO225"/>
<pin name="IO226"/>
<pin name="IO227"/>
<pin name="IO228"/>
<pin name="IO229"/>
<pin name="IO230"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO234"/>
<pin name="IO235"/>
<pin name="IO236"/>
<pin name="IO237"/>
<pin name="IO238"/>
<pin name="IO239"/>
<pin name="IO240"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO244"/>
<pin name="IO245"/>
<pin name="IO246"/>
<pin name="IO247"/>
<pin name="IO248"/>
<pin name="IO249"/>
<pin name="IO250"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO254"/>
<pin name="IO255"/>
<pin name="IO256"/>
</symbol>
<symbol name="EPM7032">
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4/TDI"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="IO8"/>
<pin name="IO9/TMS"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO20/TCK"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25/TDO"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="PD/_VCC" direction="pas"/>
</symbol>
<symbol name="PWR4-4">
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="PWR3-4">
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
</symbol>
<symbol name="EPM7064">
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4/TDI"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="IO8"/>
<pin name="IO9/TMS"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO20/TCK"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25/TDO"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="PD/_VCC" direction="pas"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO39"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO50"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO55"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
</symbol>
<symbol name="7064-44">
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO8/TDI"/>
<pin name="IO11"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO30"/>
<pin name="IO32/TMS"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="PD/_VCC" direction="pas"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO46"/>
<pin name="IO48/TCK"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO56/TDO"/>
<pin name="IO57"/>
<pin name="IO62"/>
<pin name="IO64"/>
</symbol>
<symbol name="PWR8-2-6">
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCIO@1" direction="pwr"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="VCCIO@4" direction="pwr"/>
<pin name="VCCIO@5" direction="pwr"/>
</symbol>
<symbol name="7064-68">
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO8/TDI"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO32/TMS"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="TCK/IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="TDO/IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO64"/>
</symbol>
<symbol name="NC">
<pin name="NC" direction="nc"/>
</symbol>
<symbol name="7096">
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO32"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO68"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO76"/>
<pin name="IO77"/>
<pin name="IO78"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO96"/>
</symbol>
<symbol name="7096-68">
<pin name="IO1"/>
<pin name="IO4"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO12"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO32"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO77"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO84"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO92"/>
<pin name="IO94"/>
<pin name="IO96"/>
</symbol>
<symbol name="7096-84">
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO32"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO76"/>
<pin name="IO77"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO94"/>
<pin name="IO96"/>
</symbol>
<symbol name="EPM7128">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO32/TDI"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO48/TMS"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO68"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO76"/>
<pin name="IO77"/>
<pin name="IO78"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="TCK/IO96"/>
<pin name="IO97"/>
<pin name="IO99"/>
<pin name="IO100"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO107"/>
<pin name="IO108"/>
<pin name="IO109"/>
<pin name="IO110"/>
<pin name="TDO/IO112"/>
<pin name="IO113"/>
<pin name="IO115"/>
<pin name="IO116"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO124"/>
<pin name="IO125"/>
<pin name="IO126"/>
<pin name="IO128"/>
</symbol>
<symbol name="7128-84">
<pin name="IO3"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO32/TDI"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO48/TMS"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO77"/>
<pin name="IO80"/>
<pin name="IO83"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="TCK/IO96"/>
<pin name="IO97"/>
<pin name="IO99"/>
<pin name="IO101"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO107"/>
<pin name="IO109"/>
<pin name="TDO/IO112"/>
<pin name="IO115"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO120"/>
<pin name="IO123"/>
<pin name="IO125"/>
<pin name="IO126"/>
<pin name="IO128"/>
</symbol>
<symbol name="7128P100">
<pin name="IO3"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO32/TDI"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO48/TMS"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO77"/>
<pin name="IO80"/>
<pin name="IO83"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="TCM/IO96"/>
<pin name="IO70"/>
<pin name="IO97"/>
<pin name="IO99"/>
<pin name="IO101"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO107"/>
<pin name="IO109"/>
<pin name="TDO/IO112"/>
<pin name="IO115"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO120"/>
<pin name="IO123"/>
<pin name="IO125"/>
<pin name="IO126"/>
<pin name="IO128"/>
<pin name="IO1"/>
<pin name="IO9"/>
<pin name="IO22"/>
<pin name="IO33"/>
<pin name="IO41"/>
<pin name="IO78"/>
<pin name="IO89"/>
<pin name="IO81"/>
<pin name="IO102"/>
<pin name="IO110"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO30"/>
<pin name="IO49"/>
<pin name="IO54"/>
<pin name="IO62"/>
</symbol>
<symbol name="PWR6-2-6">
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCIO@1" direction="pwr"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="VCCIO@4" direction="pwr"/>
<pin name="VCCIO@5" direction="pwr"/>
</symbol>
<symbol name="7128P160">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO39"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO50"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO55"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO66"/>
<pin name="IO67"/>
<pin name="IO68"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO75"/>
<pin name="IO76"/>
<pin name="IO77"/>
<pin name="IO78"/>
<pin name="IO79"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO87"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO90"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO95"/>
<pin name="IO96"/>
<pin name="IO97"/>
<pin name="IO98"/>
<pin name="IO99"/>
<pin name="IO100"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO106"/>
<pin name="IO107"/>
<pin name="IO108"/>
<pin name="IO109"/>
<pin name="IO110"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO115"/>
<pin name="IO116"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO119"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
<pin name="IO125"/>
<pin name="IO126"/>
<pin name="IO127"/>
<pin name="IO128"/>
</symbol>
<symbol name="PWR6-2-7">
<pin name="VCC" direction="pwr"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="VCCIO@1" direction="pwr"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="VCCIO@4" direction="pwr"/>
<pin name="VCCIO@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
</symbol>
<symbol name="EPM7160">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO2"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO7"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO10"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO39"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO50"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO55"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO59"/>
<pin name="IO60"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO66"/>
<pin name="IO67"/>
<pin name="IO68"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO75"/>
<pin name="IO76"/>
<pin name="IO77"/>
<pin name="IO78"/>
<pin name="IO79"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO87"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO90"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO95"/>
<pin name="IO96"/>
<pin name="IO97"/>
<pin name="IO98"/>
<pin name="IO99"/>
<pin name="IO100"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO106"/>
<pin name="IO107"/>
<pin name="IO108"/>
<pin name="IO109"/>
<pin name="IO110"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO115"/>
<pin name="IO116"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO119"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
<pin name="IO125"/>
<pin name="IO126"/>
<pin name="IO127"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO130"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO135"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO138"/>
<pin name="IO139"/>
<pin name="IO140"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO146"/>
<pin name="IO147"/>
<pin name="IO148"/>
<pin name="IO149"/>
<pin name="IO150"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO155"/>
<pin name="IO156"/>
<pin name="IO157"/>
<pin name="IO158"/>
<pin name="IO159"/>
<pin name="IO160"/>
</symbol>
<symbol name="7160-J84">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO32"/>
<pin name="IO35"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO43"/>
<pin name="IO46"/>
<pin name="IO48"/>
<pin name="IO51"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO59"/>
<pin name="IO62"/>
<pin name="IO64"/>
<pin name="IO67"/>
<pin name="IO70"/>
<pin name="IO72"/>
<pin name="IO75"/>
<pin name="IO78"/>
<pin name="IO80"/>
<pin name="IO83"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO91"/>
<pin name="IO94"/>
<pin name="IO96"/>
<pin name="IO99"/>
<pin name="IO102"/>
<pin name="IO104"/>
<pin name="IO107"/>
<pin name="IO110"/>
<pin name="IO112"/>
<pin name="IO115"/>
<pin name="IO118"/>
<pin name="IO120"/>
<pin name="IO123"/>
<pin name="IO126"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO131"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO139"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO147"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO155"/>
<pin name="IO160"/>
</symbol>
<symbol name="7160P100">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO22"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO30"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO46"/>
<pin name="IO48"/>
<pin name="IO51"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO59"/>
<pin name="IO62"/>
<pin name="IO64"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO72"/>
<pin name="IO75"/>
<pin name="IO77"/>
<pin name="IO78"/>
<pin name="IO80"/>
<pin name="IO83"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO91"/>
<pin name="IO94"/>
<pin name="IO96"/>
<pin name="IO99"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO104"/>
<pin name="IO107"/>
<pin name="IO109"/>
<pin name="IO110"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO115"/>
<pin name="IO118"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO126"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO131"/>
<pin name="IO134"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO139"/>
<pin name="IO142"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO147"/>
<pin name="IO150"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO155"/>
<pin name="IO158"/>
<pin name="IO160"/>
<pin name="IO61"/>
<pin name="IO53"/>
<pin name="IO85"/>
<pin name="IO93"/>
</symbol>
<symbol name="K10-J84">
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="TMS"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="IOA1"/>
<pin name="IOA3"/>
<pin name="IOA5"/>
<pin name="IOA8"/>
<pin name="IOA10"/>
<pin name="IOA12"/>
<pin name="IOA14"/>
<pin name="IOA16"/>
<pin name="IOB1"/>
<pin name="IOB3"/>
<pin name="IOB5"/>
<pin name="IOB7"/>
<pin name="IOB9"/>
<pin name="IOB11"/>
<pin name="IOB13"/>
<pin name="IOB15"/>
<pin name="IOB16"/>
<pin name="IOC1"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC7"/>
<pin name="IOC10"/>
<pin name="IOC12"/>
<pin name="IOC14"/>
<pin name="IOC16"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO22"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO43"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO71"/>
<pin name="IO91"/>
<pin name="IO102"/>
<pin name="IO112"/>
<pin name="IO123"/>
<pin name="IO133"/>
<pin name="IO141"/>
<pin name="IO151"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO181"/>
<pin name="IO191"/>
<pin name="IO201"/>
<pin name="IO211"/>
<pin name="IO223"/>
<pin name="IO233"/>
<pin name="IO243"/>
<pin name="IO244"/>
<pin name="TRST"/>
<pin name="IOA4"/>
</symbol>
<symbol name="K10-T144">
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="TMS"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOA14"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB13"/>
<pin name="IOB15"/>
<pin name="IOB16"/>
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC10"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC14"/>
<pin name="IOC15"/>
<pin name="IOC16"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO71"/>
<pin name="IO73"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO131"/>
<pin name="IO133"/>
<pin name="IO141"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO153"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO191"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO203"/>
<pin name="IO211"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO243"/>
<pin name="IO244"/>
<pin name="IO124"/>
<pin name="IO194"/>
</symbol>
<symbol name="K10-T100">
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="TMS"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA5"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA10"/>
<pin name="IOA12"/>
<pin name="IOA14"/>
<pin name="IOA16"/>
<pin name="IOB1"/>
<pin name="IOB3"/>
<pin name="IOB5"/>
<pin name="IOB7"/>
<pin name="IOB9"/>
<pin name="IOB11"/>
<pin name="IOB13"/>
<pin name="IOB15"/>
<pin name="IOB16"/>
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC7"/>
<pin name="IOC10"/>
<pin name="IOC12"/>
<pin name="IOC14"/>
<pin name="IOC16"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO43"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO71"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO102"/>
<pin name="IO112"/>
<pin name="IO123"/>
<pin name="IO133"/>
<pin name="IO141"/>
<pin name="IO151"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO181"/>
<pin name="IO191"/>
<pin name="IO201"/>
<pin name="IO211"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO233"/>
<pin name="IO243"/>
<pin name="IO244"/>
<pin name="IO124"/>
<pin name="IO194"/>
</symbol>
<symbol name="VCCINT">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="VCC">
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="VCCIO">
<pin name="VCCIO" direction="pwr"/>
</symbol>
<symbol name="GNDIO">
<pin name="GNDIO" direction="pwr"/>
</symbol>
<symbol name="GNDINT">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="K20-T144">
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="TMS"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="IOA4"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB9"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC11"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD10"/>
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE4"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE9"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF6"/>
<pin name="IOF9"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO52"/>
<pin name="IO54"/>
<pin name="IO61"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO74"/>
<pin name="IO82"/>
<pin name="IO84"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO112"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO171"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO191"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO211"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO241"/>
<pin name="IO244"/>
</symbol>
<symbol name="K30-Q144">
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="TMS"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="IOA5"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA13"/>
<pin name="IOB3"/>
<pin name="IOB6"/>
<pin name="IOB9"/>
<pin name="IOB12"/>
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC11"/>
<pin name="IOC14"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD4"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD12"/>
<pin name="IOD14"/>
<pin name="IOE1"/>
<pin name="IOE3"/>
<pin name="IOE5"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE11"/>
<pin name="IOE14"/>
<pin name="IOF1"/>
<pin name="IOF3"/>
<pin name="IOF5"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF11"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO43"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO73"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO111"/>
<pin name="IO121"/>
<pin name="IO133"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO161"/>
<pin name="IO173"/>
<pin name="IO183"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO211"/>
<pin name="IO223"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO251"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO303"/>
<pin name="IO311"/>
<pin name="IO313"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO343"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO363"/>
</symbol>
<symbol name="K30E-144">
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="TMS"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA9"/>
<pin name="IOB2"/>
<pin name="IOB6"/>
<pin name="IOB9"/>
<pin name="IOB11"/>
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC9"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD4"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE4"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF8"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO22"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO61"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO111"/>
<pin name="IO121"/>
<pin name="IO132"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO161"/>
<pin name="IO172"/>
<pin name="IO181"/>
<pin name="IO192"/>
<pin name="IO201"/>
<pin name="IO211"/>
<pin name="IO222"/>
<pin name="IO232"/>
<pin name="IO241"/>
<pin name="IO251"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO281"/>
<pin name="IO283"/>
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO303"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO322"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO343"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
</symbol>
<symbol name="7256R208">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO77-TDI"/>
<pin name="IO78"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO96"/>
<pin name="IO97"/>
<pin name="IO99"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO107"/>
<pin name="IO109-TMS"/>
<pin name="IO110"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO115"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO125"/>
<pin name="IO126"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO131"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO139"/>
<pin name="TDO-IO141"/>
<pin name="IO142"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO147"/>
<pin name="IO149"/>
<pin name="IO150"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO155"/>
<pin name="IO157"/>
<pin name="IO158"/>
<pin name="IO160"/>
<pin name="IO161"/>
<pin name="IO163"/>
<pin name="IO165"/>
<pin name="IO166"/>
<pin name="IO168"/>
<pin name="IO169"/>
<pin name="IO171"/>
<pin name="TCK-IO173"/>
<pin name="IO174"/>
<pin name="IO176"/>
<pin name="IO177"/>
<pin name="IO179"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO184"/>
<pin name="IO185"/>
<pin name="IO187"/>
<pin name="IO189"/>
<pin name="IO190"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO195"/>
<pin name="IO197"/>
<pin name="IO198"/>
<pin name="IO200"/>
<pin name="IO201"/>
<pin name="IO203"/>
<pin name="IO205"/>
<pin name="IO206"/>
<pin name="IO208"/>
<pin name="IO209"/>
<pin name="IO211"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO216"/>
<pin name="IO217"/>
<pin name="IO219"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO224"/>
<pin name="IO225"/>
<pin name="IO227"/>
<pin name="IO229"/>
<pin name="IO230"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO235"/>
<pin name="IO237"/>
<pin name="IO238"/>
<pin name="IO240"/>
<pin name="IO241"/>
<pin name="IO243"/>
<pin name="IO245"/>
<pin name="IO246"/>
<pin name="IO248"/>
<pin name="IO249"/>
<pin name="IO251"/>
<pin name="IO253"/>
<pin name="IO254"/>
<pin name="IO256"/>
</symbol>
<symbol name="7256P160">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO5"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO77-TDI"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO85"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO96"/>
<pin name="IO97"/>
<pin name="IO99"/>
<pin name="IO101"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO107"/>
<pin name="IO109-TMS"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO115"/>
<pin name="IO117"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO125"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO131"/>
<pin name="IO133"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO139"/>
<pin name="TDO-IO141"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO147"/>
<pin name="IO149"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO155"/>
<pin name="IO157"/>
<pin name="IO160"/>
<pin name="IO163"/>
<pin name="IO165"/>
<pin name="IO168"/>
<pin name="IO169"/>
<pin name="IO171"/>
<pin name="TCK-IO173"/>
<pin name="IO176"/>
<pin name="IO177"/>
<pin name="IO179"/>
<pin name="IO181"/>
<pin name="IO184"/>
<pin name="IO185"/>
<pin name="IO187"/>
<pin name="IO189"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO195"/>
<pin name="IO197"/>
<pin name="IO200"/>
<pin name="IO201"/>
<pin name="IO203"/>
<pin name="IO205"/>
<pin name="IO208"/>
<pin name="IO209"/>
<pin name="IO211"/>
<pin name="IO213"/>
<pin name="IO216"/>
<pin name="IO217"/>
<pin name="IO219"/>
<pin name="IO221"/>
<pin name="IO224"/>
<pin name="IO225"/>
<pin name="IO227"/>
<pin name="IO229"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO235"/>
<pin name="IO237"/>
<pin name="IO240"/>
<pin name="IO241"/>
<pin name="IO243"/>
<pin name="IO245"/>
<pin name="IO248"/>
<pin name="IO249"/>
<pin name="IO251"/>
<pin name="IO253"/>
<pin name="IO256"/>
<pin name="IO161"/>
</symbol>
<symbol name="7160P160">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO5"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO77-TDI"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO85"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO96"/>
<pin name="IO97"/>
<pin name="IO99"/>
<pin name="IO101"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO107"/>
<pin name="IO109-TMS"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO115"/>
<pin name="IO117"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO125"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO131"/>
<pin name="IO133"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO139"/>
<pin name="TDO-IO141"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO147"/>
<pin name="IO149"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO155"/>
<pin name="IO157"/>
<pin name="IO160"/>
<pin name="IO6"/>
<pin name="IO14"/>
<pin name="IO22"/>
<pin name="IO30"/>
<pin name="IO38"/>
<pin name="IO46"/>
<pin name="IO54"/>
<pin name="IO62"/>
<pin name="IO70"/>
<pin name="IO78"/>
<pin name="IO86"/>
<pin name="IO94"/>
<pin name="IO102"/>
<pin name="IO110"/>
<pin name="IO118"/>
<pin name="IO126"/>
<pin name="IO134"/>
<pin name="IO142"/>
<pin name="IO150"/>
<pin name="IO158"/>
</symbol>
<symbol name="7192">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO5"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO77"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO85"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO96"/>
<pin name="IO97"/>
<pin name="IO99"/>
<pin name="IO101"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO107"/>
<pin name="IO109"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO115"/>
<pin name="IO117"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO125"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO131"/>
<pin name="IO133"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO139"/>
<pin name="IO141"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO147"/>
<pin name="IO149"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO155"/>
<pin name="IO157"/>
<pin name="IO160"/>
<pin name="IO6"/>
<pin name="IO14"/>
<pin name="IO22"/>
<pin name="IO30"/>
<pin name="IO38"/>
<pin name="IO46"/>
<pin name="IO54"/>
<pin name="IO62"/>
<pin name="IO70"/>
<pin name="IO78"/>
<pin name="IO86"/>
<pin name="IO94"/>
<pin name="IO102"/>
<pin name="IO110"/>
<pin name="IO118"/>
<pin name="IO126"/>
<pin name="IO134"/>
<pin name="IO142"/>
<pin name="IO150"/>
<pin name="IO158"/>
<pin name="IO161"/>
<pin name="IO163"/>
<pin name="IO165"/>
<pin name="IO166"/>
<pin name="IO168"/>
<pin name="IO169"/>
<pin name="IO171"/>
<pin name="IO173"/>
<pin name="IO174"/>
<pin name="IO176"/>
<pin name="IO177"/>
<pin name="IO179"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO184"/>
<pin name="IO185"/>
<pin name="IO187"/>
<pin name="IO189"/>
<pin name="IO190"/>
<pin name="IO192"/>
</symbol>
<symbol name="9560C356">
<pin name="GCLR/" direction="in"/>
<pin name="VPP-1" direction="in"/>
<pin name="OE/" direction="in"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TCK"/>
<pin name="TMS"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
</symbol>
<symbol name="G16-0">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOG12"/>
<pin name="IOG13"/>
<pin name="IOG14"/>
<pin name="IOG15"/>
<pin name="IOG16"/>
</symbol>
<symbol name="IO120">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO18"/>
<pin name="IO19"/>
<pin name="IO110"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO115"/>
<pin name="IO116"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO119"/>
<pin name="IO120"/>
</symbol>
<symbol name="IO220">
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO28"/>
<pin name="IO29"/>
<pin name="IO210"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO215"/>
<pin name="IO216"/>
<pin name="IO217"/>
<pin name="IO218"/>
<pin name="IO219"/>
<pin name="IO220"/>
</symbol>
<symbol name="IO320">
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO39"/>
<pin name="IO310"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO314"/>
<pin name="IO315"/>
<pin name="IO316"/>
<pin name="IO317"/>
<pin name="IO318"/>
<pin name="IO319"/>
<pin name="IO320"/>
</symbol>
<symbol name="IO420">
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO410"/>
<pin name="IO411"/>
<pin name="IO412"/>
<pin name="IO413"/>
<pin name="IO414"/>
<pin name="IO415"/>
<pin name="IO416"/>
<pin name="IO417"/>
<pin name="IO418"/>
<pin name="IO419"/>
<pin name="IO420"/>
</symbol>
<symbol name="IO520">
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO55"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO59"/>
<pin name="IO510"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO513"/>
<pin name="IO514"/>
<pin name="IO515"/>
<pin name="IO516"/>
<pin name="IO517"/>
<pin name="IO518"/>
<pin name="IO519"/>
<pin name="IO520"/>
</symbol>
<symbol name="A16-0">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOA14"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
</symbol>
<symbol name="B16-0">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB13"/>
<pin name="IOB14"/>
<pin name="IOB15"/>
<pin name="IOB16"/>
</symbol>
<symbol name="C16-0">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC14"/>
<pin name="IOC15"/>
<pin name="IOC16"/>
</symbol>
<symbol name="D16-0">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
<pin name="IOD14"/>
<pin name="IOD15"/>
<pin name="IOD16"/>
</symbol>
<symbol name="E16-0">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
<pin name="IOE15"/>
<pin name="IOE16"/>
</symbol>
<symbol name="F16-0">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
<pin name="IOF15"/>
<pin name="IOF16"/>
</symbol>
<symbol name="IO120-1">
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO110"/>
<pin name="IO111"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO115"/>
<pin name="IO116"/>
<pin name="IO117"/>
<pin name="IO119"/>
<pin name="IO120"/>
</symbol>
<symbol name="IO220-1">
<pin name="IO21"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO210"/>
<pin name="IO211"/>
<pin name="IO213"/>
<pin name="IO215"/>
<pin name="IO216"/>
<pin name="IO217"/>
<pin name="IO219"/>
<pin name="IO220"/>
</symbol>
<symbol name="IO320-1">
<pin name="IO31"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO39"/>
<pin name="IO310"/>
<pin name="IO311"/>
<pin name="IO313"/>
<pin name="IO314"/>
<pin name="IO315"/>
<pin name="IO316"/>
<pin name="IO317"/>
<pin name="IO319"/>
<pin name="IO320"/>
</symbol>
<symbol name="IO420-1">
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO49"/>
<pin name="IO410"/>
<pin name="IO411"/>
<pin name="IO413"/>
<pin name="IO415"/>
<pin name="IO416"/>
<pin name="IO417"/>
<pin name="IO419"/>
<pin name="IO420"/>
</symbol>
<symbol name="IO520-1">
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO510"/>
<pin name="IO512"/>
<pin name="IO513"/>
<pin name="IO514"/>
<pin name="IO516"/>
<pin name="IO517"/>
<pin name="IO518"/>
<pin name="IO519"/>
<pin name="IO520"/>
</symbol>
<symbol name="A7">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
</symbol>
<symbol name="B7">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
</symbol>
<symbol name="C7">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
</symbol>
<symbol name="D7">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
</symbol>
<symbol name="E7">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
</symbol>
<symbol name="F7">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
</symbol>
<symbol name="G7">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
</symbol>
<symbol name="IO120-2">
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO15"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO110"/>
<pin name="IO111"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO115"/>
<pin name="IO116"/>
<pin name="IO117"/>
<pin name="IO119"/>
<pin name="IO120"/>
</symbol>
<symbol name="IO320-2">
<pin name="IO31"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO39"/>
<pin name="IO310"/>
<pin name="IO311"/>
<pin name="IO313"/>
<pin name="IO314"/>
<pin name="IO315"/>
<pin name="IO316"/>
<pin name="IO317"/>
<pin name="IO319"/>
<pin name="IO320"/>
</symbol>
<symbol name="IO420-2">
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO47"/>
<pin name="IO49"/>
<pin name="IO410"/>
<pin name="IO411"/>
<pin name="IO413"/>
<pin name="IO415"/>
<pin name="IO416"/>
<pin name="IO417"/>
<pin name="IO419"/>
<pin name="IO420"/>
</symbol>
<symbol name="IO220-2">
<pin name="IO21"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO26"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO210"/>
<pin name="IO211"/>
<pin name="IO213"/>
<pin name="IO215"/>
<pin name="IO216"/>
<pin name="IO217"/>
<pin name="IO219"/>
<pin name="IO220"/>
</symbol>
<symbol name="IO520-2">
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO58"/>
<pin name="IO510"/>
<pin name="IO512"/>
<pin name="IO513"/>
<pin name="IO514"/>
<pin name="IO516"/>
<pin name="IO517"/>
<pin name="IO518"/>
<pin name="IO519"/>
<pin name="IO520"/>
</symbol>
<symbol name="K10-CTRL">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="A16">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOA14"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
</symbol>
<symbol name="B16">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB13"/>
<pin name="IOB14"/>
<pin name="IOB15"/>
<pin name="IOB16"/>
</symbol>
<symbol name="C16">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC14"/>
<pin name="IOC15"/>
<pin name="IOC16"/>
</symbol>
<symbol name="IO-44">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
</symbol>
<symbol name="IO-84">
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
</symbol>
<symbol name="IO-124">
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
</symbol>
<symbol name="IO-164">
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
</symbol>
<symbol name="IO-204">
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO174"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO194"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
</symbol>
<symbol name="IO-244">
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO224"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO234"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO244"/>
</symbol>
<symbol name="100-524">
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO504"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO521"/>
<pin name="IO522"/>
<pin name="IO524"/>
</symbol>
<symbol name="100B356C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="100A16">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA12"/>
<pin name="IOA14"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
</symbol>
<symbol name="100B16">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB12"/>
<pin name="IOB16"/>
</symbol>
<symbol name="100C16">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC15"/>
<pin name="IOC16"/>
</symbol>
<symbol name="100D16">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD12"/>
<pin name="IOD14"/>
<pin name="IOD15"/>
<pin name="IOD16"/>
</symbol>
<symbol name="100E16">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE11"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
<pin name="IOE16"/>
</symbol>
<symbol name="100F15">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
<pin name="IOF15"/>
</symbol>
<symbol name="100G16">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOG12"/>
<pin name="IOG13"/>
<pin name="IOG15"/>
<pin name="IOG16"/>
</symbol>
<symbol name="100H16">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH11"/>
<pin name="IOH12"/>
<pin name="IOH13"/>
<pin name="IOH14"/>
<pin name="IOH16"/>
</symbol>
<symbol name="100I16">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI12"/>
<pin name="IOI13"/>
<pin name="IOI14"/>
<pin name="IOI15"/>
<pin name="IOI16"/>
</symbol>
<symbol name="100J15">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="IOJ12"/>
<pin name="IOJ13"/>
<pin name="IOJ14"/>
<pin name="IOJ15"/>
</symbol>
<symbol name="100K15">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
<pin name="IOK14"/>
<pin name="IOK15"/>
</symbol>
<symbol name="100L16">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL10"/>
<pin name="IOL11"/>
<pin name="IOL12"/>
<pin name="IOL13"/>
<pin name="IOL15"/>
<pin name="IOL16"/>
</symbol>
<symbol name="100-113">
<pin name="IO11"/>
<pin name="IO21"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO42"/>
<pin name="IO51"/>
<pin name="IO61"/>
<pin name="IO71"/>
<pin name="IO73"/>
<pin name="IO81"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO113"/>
</symbol>
<symbol name="100-181">
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO124"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO181"/>
</symbol>
<symbol name="100-242">
<pin name="IO182"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO194"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO234"/>
<pin name="IO241"/>
<pin name="IO242"/>
</symbol>
<symbol name="100-311">
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO261"/>
<pin name="IO263"/>
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO284"/>
<pin name="IO291"/>
<pin name="IO294"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
</symbol>
<symbol name="100-402">
<pin name="IO321"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO351"/>
<pin name="IO353"/>
<pin name="IO361"/>
<pin name="IO364"/>
<pin name="IO371"/>
<pin name="IO372"/>
<pin name="IO381"/>
<pin name="IO391"/>
<pin name="IO392"/>
<pin name="IO401"/>
<pin name="IO402"/>
</symbol>
<symbol name="100-473">
<pin name="IO404"/>
<pin name="IO411"/>
<pin name="IO413"/>
<pin name="IO414"/>
<pin name="IO421"/>
<pin name="IO423"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO441"/>
<pin name="IO443"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO471"/>
<pin name="IO473"/>
</symbol>
<symbol name="L484">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL8"/>
<pin name="IOL10"/>
<pin name="IOL11"/>
<pin name="IOL12"/>
<pin name="IOL13"/>
<pin name="IOL14"/>
<pin name="IOL15"/>
<pin name="IOL16"/>
</symbol>
<symbol name="100B484C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="IO51">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO44"/>
<pin name="IO51"/>
</symbol>
<symbol name="IO92">
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO91"/>
<pin name="IO92"/>
</symbol>
<symbol name="IO133">
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
</symbol>
<symbol name="IO173">
<pin name="IO134"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
</symbol>
<symbol name="IO214">
<pin name="IO174"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO194"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
</symbol>
<symbol name="IO254">
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO224"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO234"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO244"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO254"/>
</symbol>
<symbol name="IO302">
<pin name="IO261"/>
<pin name="IO263"/>
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO274"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO284"/>
<pin name="IO291"/>
<pin name="IO293"/>
<pin name="IO294"/>
<pin name="IO301"/>
<pin name="IO302"/>
</symbol>
<symbol name="IO353">
<pin name="IO303"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO343"/>
<pin name="IO344"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
</symbol>
<symbol name="IO401">
<pin name="IO354"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
<pin name="IO364"/>
<pin name="IO371"/>
<pin name="IO372"/>
<pin name="IO373"/>
<pin name="IO374"/>
<pin name="IO381"/>
<pin name="IO383"/>
<pin name="IO384"/>
<pin name="IO391"/>
<pin name="IO392"/>
<pin name="IO394"/>
<pin name="IO401"/>
</symbol>
<symbol name="IO443">
<pin name="IO402"/>
<pin name="IO404"/>
<pin name="IO411"/>
<pin name="IO412"/>
<pin name="IO413"/>
<pin name="IO414"/>
<pin name="IO421"/>
<pin name="IO423"/>
<pin name="IO424"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO433"/>
<pin name="IO434"/>
<pin name="IO441"/>
<pin name="IO442"/>
<pin name="IO443"/>
</symbol>
<symbol name="IO483">
<pin name="IO444"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO453"/>
<pin name="IO454"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO463"/>
<pin name="IO464"/>
<pin name="IO471"/>
<pin name="IO472"/>
<pin name="IO473"/>
<pin name="IO474"/>
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO483"/>
</symbol>
<symbol name="IO524">
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO493"/>
<pin name="IO494"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO503"/>
<pin name="IO504"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO513"/>
<pin name="IO514"/>
<pin name="IO521"/>
<pin name="IO522"/>
<pin name="IO523"/>
<pin name="IO524"/>
</symbol>
<symbol name="A484">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA12"/>
<pin name="IOA14"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
</symbol>
<symbol name="B484">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB12"/>
<pin name="IOB13"/>
<pin name="IOB16"/>
</symbol>
<symbol name="C484">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC15"/>
<pin name="IOC16"/>
</symbol>
<symbol name="D484">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
<pin name="IOD14"/>
<pin name="IOD15"/>
<pin name="IOD16"/>
</symbol>
<symbol name="E484">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
<pin name="IOE16"/>
</symbol>
<symbol name="F484">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
<pin name="IOF15"/>
<pin name="IOF16"/>
</symbol>
<symbol name="G484">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOG12"/>
<pin name="IOG13"/>
<pin name="IOG15"/>
<pin name="IOG16"/>
</symbol>
<symbol name="H484">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
<pin name="IOH12"/>
<pin name="IOH13"/>
<pin name="IOH14"/>
<pin name="IOH15"/>
<pin name="IOH16"/>
</symbol>
<symbol name="I484">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI11"/>
<pin name="IOI12"/>
<pin name="IOI13"/>
<pin name="IOI14"/>
<pin name="IOI15"/>
<pin name="IOI16"/>
</symbol>
<symbol name="J484">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="IOJ12"/>
<pin name="IOJ13"/>
<pin name="IOJ14"/>
<pin name="IOJ15"/>
<pin name="IOJ16"/>
</symbol>
<symbol name="K484">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
<pin name="IOK13"/>
<pin name="IOK14"/>
<pin name="IOK15"/>
</symbol>
<symbol name="OP5">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
</symbol>
<symbol name="K_CTRL">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="122-240">
<pin name="IO11"/>
<pin name="IO21"/>
<pin name="IO31"/>
<pin name="IO41"/>
<pin name="IO51"/>
<pin name="IO61"/>
<pin name="IO71"/>
<pin name="IO81"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO121"/>
<pin name="IO122"/>
</symbol>
<symbol name="192-240">
<pin name="IO123"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO171"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO191"/>
<pin name="IO192"/>
</symbol>
<symbol name="261-240">
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO261"/>
</symbol>
<symbol name="322-240">
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
<pin name="IO321"/>
<pin name="IO322"/>
</symbol>
<symbol name="403-240">
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
<pin name="IO371"/>
<pin name="IO381"/>
<pin name="IO382"/>
<pin name="IO391"/>
<pin name="IO401"/>
<pin name="IO402"/>
<pin name="IO403"/>
</symbol>
<symbol name="511-240">
<pin name="IO411"/>
<pin name="IO421"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO441"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO471"/>
<pin name="IO481"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO511"/>
</symbol>
<symbol name="522-240">
<pin name="IO512"/>
<pin name="IO521"/>
<pin name="IO522"/>
</symbol>
<symbol name="AB6">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
</symbol>
<symbol name="CD6">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
</symbol>
<symbol name="EF6">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
</symbol>
<symbol name="GH6">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
</symbol>
<symbol name="IJ4">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
</symbol>
<symbol name="KL4">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
</symbol>
<symbol name="MN4">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM4"/>
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
</symbol>
<symbol name="KL-256">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK11"/>
<pin name="IOK14"/>
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL7"/>
<pin name="IOL11"/>
</symbol>
<symbol name="100F256C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="122-256">
<pin name="IO11"/>
<pin name="IO21"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO41"/>
<pin name="IO51"/>
<pin name="IO61"/>
<pin name="IO71"/>
<pin name="IO81"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO101"/>
<pin name="IO111"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
</symbol>
<symbol name="192-256">
<pin name="IO124"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO164"/>
<pin name="IO171"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO191"/>
<pin name="IO192"/>
</symbol>
<symbol name="261-256">
<pin name="IO194"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO234"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO261"/>
</symbol>
<symbol name="323-256">
<pin name="IO263"/>
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO284"/>
<pin name="IO291"/>
<pin name="IO293"/>
<pin name="IO294"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
<pin name="IO321"/>
<pin name="IO323"/>
</symbol>
<symbol name="411-256">
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
<pin name="IO361"/>
<pin name="IO364"/>
<pin name="IO371"/>
<pin name="IO372"/>
<pin name="IO381"/>
<pin name="IO391"/>
<pin name="IO402"/>
<pin name="IO404"/>
<pin name="IO411"/>
</symbol>
<symbol name="504-256">
<pin name="IO421"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO441"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO471"/>
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO504"/>
</symbol>
<symbol name="522-256">
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO521"/>
<pin name="IO522"/>
</symbol>
<symbol name="AB-256">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB16"/>
</symbol>
<symbol name="CD-256">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC11"/>
<pin name="IOC16"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
</symbol>
<symbol name="EF-256">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE13"/>
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF7"/>
<pin name="IOF14"/>
</symbol>
<symbol name="GH-256">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG6"/>
<pin name="IOG8"/>
<pin name="IOG11"/>
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH8"/>
</symbol>
<symbol name="IJ-256">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI5"/>
<pin name="IOI12"/>
<pin name="IOI14"/>
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ10"/>
<pin name="IOJ14"/>
<pin name="IOJ15"/>
</symbol>
<symbol name="K200-CTR">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="X10-672">
<pin name="IOX1"/>
<pin name="IOX2"/>
<pin name="IOX3"/>
<pin name="IOX4"/>
<pin name="IOX5"/>
<pin name="IOX6"/>
<pin name="IOX7"/>
<pin name="IOX8"/>
<pin name="IOX9"/>
<pin name="IOX10"/>
</symbol>
<symbol name="IO44">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
</symbol>
<symbol name="IO84">
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
</symbol>
<symbol name="IO204">
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO174"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO194"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
</symbol>
<symbol name="IO244">
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO224"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO234"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO244"/>
</symbol>
<symbol name="IO284">
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO254"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO274"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO284"/>
</symbol>
<symbol name="IO124">
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
</symbol>
<symbol name="IO164">
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
</symbol>
<symbol name="IO324">
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO294"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO303"/>
<pin name="IO304"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO314"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO324"/>
</symbol>
<symbol name="IO364">
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO334"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO344"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
<pin name="IO354"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
<pin name="IO364"/>
</symbol>
<symbol name="IO404">
<pin name="IO371"/>
<pin name="IO372"/>
<pin name="IO373"/>
<pin name="IO374"/>
<pin name="IO381"/>
<pin name="IO382"/>
<pin name="IO383"/>
<pin name="IO384"/>
<pin name="IO391"/>
<pin name="IO392"/>
<pin name="IO393"/>
<pin name="IO394"/>
<pin name="IO401"/>
<pin name="IO402"/>
<pin name="IO403"/>
<pin name="IO404"/>
</symbol>
<symbol name="IO444">
<pin name="IO411"/>
<pin name="IO412"/>
<pin name="IO413"/>
<pin name="IO414"/>
<pin name="IO421"/>
<pin name="IO422"/>
<pin name="IO423"/>
<pin name="IO424"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO433"/>
<pin name="IO434"/>
<pin name="IO441"/>
<pin name="IO442"/>
<pin name="IO443"/>
<pin name="IO444"/>
</symbol>
<symbol name="IO484">
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO453"/>
<pin name="IO454"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO463"/>
<pin name="IO464"/>
<pin name="IO471"/>
<pin name="IO472"/>
<pin name="IO473"/>
<pin name="IO474"/>
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO483"/>
<pin name="IO484"/>
</symbol>
<symbol name="A11-672">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
</symbol>
<symbol name="B11-672">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
</symbol>
<symbol name="C10-672">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
</symbol>
<symbol name="D11-672">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
</symbol>
<symbol name="E11-672">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE11"/>
</symbol>
<symbol name="F10-672">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
</symbol>
<symbol name="G11-672">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
</symbol>
<symbol name="H11-672">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
</symbol>
<symbol name="I11-672">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI8"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI11"/>
</symbol>
<symbol name="J13-672">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ12"/>
<pin name="IOJ13"/>
</symbol>
<symbol name="K11-672">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
</symbol>
<symbol name="L10-672">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
</symbol>
<symbol name="M11-672">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM4"/>
<pin name="IOM5"/>
<pin name="IOM6"/>
<pin name="IOM7"/>
<pin name="IOM8"/>
<pin name="IOM9"/>
<pin name="IOM10"/>
<pin name="IOM11"/>
</symbol>
<symbol name="N11-672">
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="ION5"/>
<pin name="ION6"/>
<pin name="ION7"/>
<pin name="ION8"/>
<pin name="ION9"/>
<pin name="ION10"/>
<pin name="ION11"/>
</symbol>
<symbol name="O10-672">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOO5"/>
<pin name="IOO6"/>
<pin name="IOO7"/>
<pin name="IOO8"/>
<pin name="IOO9"/>
<pin name="IOO10"/>
</symbol>
<symbol name="P11-672">
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
<pin name="IOP6"/>
<pin name="IOP7"/>
<pin name="IOP8"/>
<pin name="IOP9"/>
<pin name="IOP10"/>
<pin name="IOP11"/>
</symbol>
<symbol name="Q11-672">
<pin name="IOQ1"/>
<pin name="IOQ2"/>
<pin name="IOQ3"/>
<pin name="IOQ4"/>
<pin name="IOQ5"/>
<pin name="IOQ6"/>
<pin name="IOQ7"/>
<pin name="IOQ8"/>
<pin name="IOQ9"/>
<pin name="IOQ10"/>
<pin name="IOQ11"/>
</symbol>
<symbol name="R10-672">
<pin name="IOR1"/>
<pin name="IOR2"/>
<pin name="IOR3"/>
<pin name="IOR4"/>
<pin name="IOR5"/>
<pin name="IOR6"/>
<pin name="IOR7"/>
<pin name="IOR8"/>
<pin name="IOR9"/>
<pin name="IOR10"/>
</symbol>
<symbol name="S11-672">
<pin name="IOS1"/>
<pin name="IOS2"/>
<pin name="IOS3"/>
<pin name="IOS4"/>
<pin name="IOS5"/>
<pin name="IOS6"/>
<pin name="IOS7"/>
<pin name="IOS8"/>
<pin name="IOS9"/>
<pin name="IOS10"/>
<pin name="IOS11"/>
</symbol>
<symbol name="T11-672">
<pin name="IOT1"/>
<pin name="IOT2"/>
<pin name="IOT3"/>
<pin name="IOT4"/>
<pin name="IOT5"/>
<pin name="IOT6"/>
<pin name="IOT7"/>
<pin name="IOT8"/>
<pin name="IOT9"/>
<pin name="IOT10"/>
<pin name="IOT11"/>
</symbol>
<symbol name="V11-672">
<pin name="IOV1"/>
<pin name="IOV2"/>
<pin name="IOV3"/>
<pin name="IOV4"/>
<pin name="IOV5"/>
<pin name="IOV6"/>
<pin name="IOV7"/>
<pin name="IOV8"/>
<pin name="IOV9"/>
<pin name="IOV10"/>
<pin name="IOV11"/>
</symbol>
<symbol name="W11-672">
<pin name="IOW1"/>
<pin name="IOW2"/>
<pin name="IOW3"/>
<pin name="IOW4"/>
<pin name="IOW5"/>
<pin name="IOW6"/>
<pin name="IOW7"/>
<pin name="IOW8"/>
<pin name="IOW9"/>
<pin name="IOW10"/>
<pin name="IOW11"/>
</symbol>
<symbol name="U10-672">
<pin name="IOU1"/>
<pin name="IOU2"/>
<pin name="IOU3"/>
<pin name="IOU4"/>
<pin name="IOU5"/>
<pin name="IOU6"/>
<pin name="IOU7"/>
<pin name="IOU8"/>
<pin name="IOU9"/>
<pin name="IOU10"/>
</symbol>
<symbol name="K250_C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="A13-250">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
</symbol>
<symbol name="B12-250">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
</symbol>
<symbol name="C13-250">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
</symbol>
<symbol name="D13-250">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
</symbol>
<symbol name="E12-250">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
</symbol>
<symbol name="F12-250">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
</symbol>
<symbol name="G13-250">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOG12"/>
<pin name="IOG13"/>
</symbol>
<symbol name="H12-250">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
<pin name="IOH12"/>
</symbol>
<symbol name="I13-250">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI8"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI11"/>
<pin name="IOI12"/>
<pin name="IOI13"/>
</symbol>
<symbol name="J13-250">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="IOJ12"/>
<pin name="IOJ13"/>
</symbol>
<symbol name="K12-250">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
<pin name="IOK12"/>
</symbol>
<symbol name="L12-250">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
<pin name="IOL11"/>
<pin name="IOL12"/>
</symbol>
<symbol name="M13-250">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM4"/>
<pin name="IOM5"/>
<pin name="IOM6"/>
<pin name="IOM7"/>
<pin name="IOM8"/>
<pin name="IOM9"/>
<pin name="IOM10"/>
<pin name="IOM11"/>
<pin name="IOM12"/>
<pin name="IOM13"/>
</symbol>
<symbol name="N13-250">
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="ION5"/>
<pin name="ION6"/>
<pin name="ION7"/>
<pin name="ION8"/>
<pin name="ION9"/>
<pin name="ION10"/>
<pin name="ION11"/>
<pin name="ION12"/>
<pin name="ION13"/>
</symbol>
<symbol name="O13-250">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOO5"/>
<pin name="IOO6"/>
<pin name="IOO7"/>
<pin name="IOO8"/>
<pin name="IOO9"/>
<pin name="IOO10"/>
<pin name="IOO11"/>
<pin name="IOO12"/>
<pin name="IOO13"/>
</symbol>
<symbol name="Q14-250">
<pin name="IOQ2"/>
<pin name="IOQ3"/>
<pin name="IOQ4"/>
<pin name="IOQ5"/>
<pin name="IOQ6"/>
<pin name="IOQ7"/>
<pin name="IOQ8"/>
<pin name="IOQ9"/>
<pin name="IOQ10"/>
<pin name="IOQ11"/>
<pin name="IOQ12"/>
<pin name="IOQ13"/>
<pin name="IOQ14"/>
<pin name="IOQ1"/>
</symbol>
<symbol name="R12-250">
<pin name="IOR1"/>
<pin name="IOR2"/>
<pin name="IOR3"/>
<pin name="IOR4"/>
<pin name="IOR5"/>
<pin name="IOR6"/>
<pin name="IOR7"/>
<pin name="IOR8"/>
<pin name="IOR9"/>
<pin name="IOR10"/>
<pin name="IOR11"/>
<pin name="IOR12"/>
</symbol>
<symbol name="S13-250">
<pin name="IOS1"/>
<pin name="IOS2"/>
<pin name="IOS3"/>
<pin name="IOS4"/>
<pin name="IOS5"/>
<pin name="IOS6"/>
<pin name="IOS7"/>
<pin name="IOS8"/>
<pin name="IOS9"/>
<pin name="IOS10"/>
<pin name="IOS11"/>
<pin name="IOS12"/>
<pin name="IOS13"/>
</symbol>
<symbol name="T14-250">
<pin name="IOT1"/>
<pin name="IOT2"/>
<pin name="IOT3"/>
<pin name="IOT4"/>
<pin name="IOT5"/>
<pin name="IOT6"/>
<pin name="IOT7"/>
<pin name="IOT8"/>
<pin name="IOT9"/>
<pin name="IOT10"/>
<pin name="IOT11"/>
<pin name="IOT12"/>
<pin name="IOT13"/>
<pin name="IOT14"/>
</symbol>
<symbol name="62-250">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
</symbol>
<symbol name="122-250">
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
</symbol>
<symbol name="182-250">
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO181"/>
<pin name="IO182"/>
</symbol>
<symbol name="242-250">
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
</symbol>
<symbol name="302-250">
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO302"/>
</symbol>
<symbol name="361-250">
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
<pin name="IO361"/>
</symbol>
<symbol name="412-250">
<pin name="IO362"/>
<pin name="IO363"/>
<pin name="IO371"/>
<pin name="IO372"/>
<pin name="IO373"/>
<pin name="IO381"/>
<pin name="IO382"/>
<pin name="IO383"/>
<pin name="IO391"/>
<pin name="IO392"/>
<pin name="IO393"/>
<pin name="IO401"/>
<pin name="IO402"/>
<pin name="IO403"/>
<pin name="IO411"/>
<pin name="IO412"/>
</symbol>
<symbol name="471-250">
<pin name="IO421"/>
<pin name="IO422"/>
<pin name="IO423"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO433"/>
<pin name="IO441"/>
<pin name="IO442"/>
<pin name="IO443"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO453"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO463"/>
<pin name="IO471"/>
</symbol>
<symbol name="531-250">
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO483"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO493"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO503"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO513"/>
<pin name="IO521"/>
<pin name="IO522"/>
<pin name="IO523"/>
<pin name="IO531"/>
</symbol>
<symbol name="583-250">
<pin name="IO532"/>
<pin name="IO541"/>
<pin name="IO542"/>
<pin name="IO543"/>
<pin name="IO551"/>
<pin name="IO552"/>
<pin name="IO553"/>
<pin name="IO561"/>
<pin name="IO562"/>
<pin name="IO563"/>
<pin name="IO571"/>
<pin name="IO572"/>
<pin name="IO573"/>
<pin name="IO581"/>
<pin name="IO582"/>
<pin name="IO583"/>
</symbol>
<symbol name="642-250">
<pin name="IO591"/>
<pin name="IO592"/>
<pin name="IO601"/>
<pin name="IO602"/>
<pin name="IO603"/>
<pin name="IO611"/>
<pin name="IO612"/>
<pin name="IO613"/>
<pin name="IO621"/>
<pin name="IO622"/>
<pin name="IO623"/>
<pin name="IO631"/>
<pin name="IO632"/>
<pin name="IO633"/>
<pin name="IO641"/>
<pin name="IO642"/>
</symbol>
<symbol name="702-250">
<pin name="IO651"/>
<pin name="IO652"/>
<pin name="IO661"/>
<pin name="IO662"/>
<pin name="IO663"/>
<pin name="IO671"/>
<pin name="IO672"/>
<pin name="IO673"/>
<pin name="IO681"/>
<pin name="IO682"/>
<pin name="IO683"/>
<pin name="IO691"/>
<pin name="IO692"/>
<pin name="IO693"/>
<pin name="IO701"/>
<pin name="IO702"/>
</symbol>
<symbol name="762-250">
<pin name="IO711"/>
<pin name="IO712"/>
<pin name="IO721"/>
<pin name="IO722"/>
<pin name="IO723"/>
<pin name="IO731"/>
<pin name="IO732"/>
<pin name="IO733"/>
<pin name="IO741"/>
<pin name="IO742"/>
<pin name="IO743"/>
<pin name="IO751"/>
<pin name="IO752"/>
<pin name="IO753"/>
<pin name="IO761"/>
<pin name="IO762"/>
</symbol>
<symbol name="P14-250">
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
<pin name="IOP6"/>
<pin name="IOP7"/>
<pin name="IOP8"/>
<pin name="IOP9"/>
<pin name="IOP10"/>
<pin name="IOP11"/>
<pin name="IOP12"/>
<pin name="IOP13"/>
<pin name="IOP14"/>
</symbol>
<symbol name="K240C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="A13-600">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
</symbol>
<symbol name="62-600">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
</symbol>
<symbol name="122-600">
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
</symbol>
<symbol name="182-600">
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO181"/>
<pin name="IO182"/>
</symbol>
<symbol name="242-600">
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
</symbol>
<symbol name="302-600">
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO302"/>
</symbol>
<symbol name="361-600">
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
<pin name="IO361"/>
</symbol>
<symbol name="412-600">
<pin name="IO362"/>
<pin name="IO363"/>
<pin name="IO371"/>
<pin name="IO372"/>
<pin name="IO373"/>
<pin name="IO381"/>
<pin name="IO382"/>
<pin name="IO383"/>
<pin name="IO391"/>
<pin name="IO392"/>
<pin name="IO393"/>
<pin name="IO401"/>
<pin name="IO402"/>
<pin name="IO403"/>
<pin name="IO411"/>
<pin name="IO412"/>
</symbol>
<symbol name="471-600">
<pin name="IO421"/>
<pin name="IO422"/>
<pin name="IO423"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO433"/>
<pin name="IO441"/>
<pin name="IO442"/>
<pin name="IO443"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO453"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO463"/>
<pin name="IO471"/>
</symbol>
<symbol name="531-600">
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO483"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO493"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO503"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO513"/>
<pin name="IO521"/>
<pin name="IO522"/>
<pin name="IO523"/>
<pin name="IO531"/>
</symbol>
<symbol name="583-600">
<pin name="IO532"/>
<pin name="IO541"/>
<pin name="IO542"/>
<pin name="IO543"/>
<pin name="IO551"/>
<pin name="IO552"/>
<pin name="IO553"/>
<pin name="IO561"/>
<pin name="IO562"/>
<pin name="IO563"/>
<pin name="IO571"/>
<pin name="IO572"/>
<pin name="IO573"/>
<pin name="IO581"/>
<pin name="IO582"/>
<pin name="IO583"/>
</symbol>
<symbol name="642-600">
<pin name="IO591"/>
<pin name="IO592"/>
<pin name="IO601"/>
<pin name="IO602"/>
<pin name="IO603"/>
<pin name="IO611"/>
<pin name="IO612"/>
<pin name="IO613"/>
<pin name="IO621"/>
<pin name="IO622"/>
<pin name="IO623"/>
<pin name="IO631"/>
<pin name="IO632"/>
<pin name="IO633"/>
<pin name="IO641"/>
<pin name="IO642"/>
</symbol>
<symbol name="702-600">
<pin name="IO651"/>
<pin name="IO652"/>
<pin name="IO661"/>
<pin name="IO662"/>
<pin name="IO663"/>
<pin name="IO671"/>
<pin name="IO672"/>
<pin name="IO673"/>
<pin name="IO681"/>
<pin name="IO682"/>
<pin name="IO683"/>
<pin name="IO691"/>
<pin name="IO692"/>
<pin name="IO693"/>
<pin name="IO701"/>
<pin name="IO702"/>
</symbol>
<symbol name="762-600">
<pin name="IO711"/>
<pin name="IO712"/>
<pin name="IO721"/>
<pin name="IO722"/>
<pin name="IO723"/>
<pin name="IO731"/>
<pin name="IO732"/>
<pin name="IO733"/>
<pin name="IO741"/>
<pin name="IO742"/>
<pin name="IO743"/>
<pin name="IO751"/>
<pin name="IO752"/>
<pin name="IO753"/>
<pin name="IO761"/>
<pin name="IO762"/>
</symbol>
<symbol name="B12-600">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
</symbol>
<symbol name="C13-600">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
</symbol>
<symbol name="D13-600">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
</symbol>
<symbol name="E12-600">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
</symbol>
<symbol name="F12-600">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
</symbol>
<symbol name="G13-600">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOG12"/>
<pin name="IOG13"/>
</symbol>
<symbol name="H12-600">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
<pin name="IOH12"/>
</symbol>
<symbol name="I13-600">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI8"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI11"/>
<pin name="IOI12"/>
<pin name="IOI13"/>
</symbol>
<symbol name="J13-600">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="IOJ12"/>
<pin name="IOJ13"/>
</symbol>
<symbol name="K12-600">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
<pin name="IOK12"/>
</symbol>
<symbol name="L12-600">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
<pin name="IOL11"/>
<pin name="IOL12"/>
</symbol>
<symbol name="M13-600">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM4"/>
<pin name="IOM5"/>
<pin name="IOM6"/>
<pin name="IOM7"/>
<pin name="IOM8"/>
<pin name="IOM9"/>
<pin name="IOM10"/>
<pin name="IOM11"/>
<pin name="IOM12"/>
<pin name="IOM13"/>
</symbol>
<symbol name="N13-600">
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="ION5"/>
<pin name="ION6"/>
<pin name="ION7"/>
<pin name="ION8"/>
<pin name="ION9"/>
<pin name="ION10"/>
<pin name="ION11"/>
<pin name="ION12"/>
<pin name="ION13"/>
</symbol>
<symbol name="O13-600">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOO5"/>
<pin name="IOO6"/>
<pin name="IOO7"/>
<pin name="IOO8"/>
<pin name="IOO9"/>
<pin name="IOO10"/>
<pin name="IOO11"/>
<pin name="IOO12"/>
<pin name="IOO13"/>
</symbol>
<symbol name="P14-600">
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
<pin name="IOP6"/>
<pin name="IOP7"/>
<pin name="IOP8"/>
<pin name="IOP9"/>
<pin name="IOP10"/>
<pin name="IOP11"/>
<pin name="IOP12"/>
<pin name="IOP13"/>
<pin name="IOP14"/>
</symbol>
<symbol name="Q14-600">
<pin name="IOQ1"/>
<pin name="IOQ2"/>
<pin name="IOQ3"/>
<pin name="IOQ4"/>
<pin name="IOQ5"/>
<pin name="IOQ6"/>
<pin name="IOQ7"/>
<pin name="IOQ8"/>
<pin name="IOQ9"/>
<pin name="IOQ10"/>
<pin name="IOQ11"/>
<pin name="IOQ12"/>
<pin name="IOQ13"/>
<pin name="IOQ14"/>
</symbol>
<symbol name="R12-600">
<pin name="IOR1"/>
<pin name="IOR2"/>
<pin name="IOR3"/>
<pin name="IOR4"/>
<pin name="IOR5"/>
<pin name="IOR6"/>
<pin name="IOR7"/>
<pin name="IOR8"/>
<pin name="IOR9"/>
<pin name="IOR10"/>
<pin name="IOR11"/>
<pin name="IOR12"/>
</symbol>
<symbol name="S13-600">
<pin name="IOS1"/>
<pin name="IOS2"/>
<pin name="IOS3"/>
<pin name="IOS4"/>
<pin name="IOS5"/>
<pin name="IOS6"/>
<pin name="IOS7"/>
<pin name="IOS8"/>
<pin name="IOS9"/>
<pin name="IOS10"/>
<pin name="IOS11"/>
<pin name="IOS12"/>
<pin name="IOS13"/>
</symbol>
<symbol name="T14-600">
<pin name="IOT1"/>
<pin name="IOT2"/>
<pin name="IOT3"/>
<pin name="IOT4"/>
<pin name="IOT5"/>
<pin name="IOT6"/>
<pin name="IOT7"/>
<pin name="IOT8"/>
<pin name="IOT9"/>
<pin name="IOT10"/>
<pin name="IOT11"/>
<pin name="IOT12"/>
<pin name="IOT13"/>
<pin name="IOT14"/>
</symbol>
<symbol name="WX10">
<pin name="IOW1"/>
<pin name="IOW2"/>
<pin name="IOW3"/>
<pin name="IOW4"/>
<pin name="IOW5"/>
<pin name="IOW6"/>
<pin name="IOW7"/>
<pin name="IOW8"/>
<pin name="IOW9"/>
<pin name="IOW10"/>
<pin name="IOW11"/>
<pin name="IOX1"/>
<pin name="IOX2"/>
<pin name="IOX3"/>
<pin name="IOX4"/>
<pin name="IOX5"/>
<pin name="IOX6"/>
<pin name="IOX7"/>
<pin name="IOX8"/>
<pin name="IOX9"/>
<pin name="IOX10"/>
</symbol>
<symbol name="200B600C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="AB11">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
</symbol>
<symbol name="CD11">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
</symbol>
<symbol name="EF10">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
</symbol>
<symbol name="GH11">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
</symbol>
<symbol name="IJ12">
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI8"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI11"/>
<pin name="IOJ1"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="IOJ12"/>
</symbol>
<symbol name="KL10">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
</symbol>
<symbol name="MN11">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM4"/>
<pin name="IOM5"/>
<pin name="IOM6"/>
<pin name="IOM7"/>
<pin name="IOM8"/>
<pin name="IOM9"/>
<pin name="IOM10"/>
<pin name="IOM11"/>
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="ION5"/>
<pin name="ION6"/>
<pin name="ION7"/>
<pin name="ION8"/>
<pin name="ION9"/>
<pin name="ION10"/>
<pin name="ION11"/>
</symbol>
<symbol name="OP11">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOO5"/>
<pin name="IOO6"/>
<pin name="IOO7"/>
<pin name="IOO8"/>
<pin name="IOO9"/>
<pin name="IOO10"/>
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
<pin name="IOP6"/>
<pin name="IOP7"/>
<pin name="IOP8"/>
<pin name="IOP9"/>
<pin name="IOP10"/>
<pin name="IOP11"/>
</symbol>
<symbol name="QR10">
<pin name="IOQ1"/>
<pin name="IOQ2"/>
<pin name="IOQ3"/>
<pin name="IOQ4"/>
<pin name="IOQ5"/>
<pin name="IOQ6"/>
<pin name="IOQ7"/>
<pin name="IOQ8"/>
<pin name="IOQ9"/>
<pin name="IOQ10"/>
<pin name="IOQ11"/>
<pin name="IOR1"/>
<pin name="IOR2"/>
<pin name="IOR3"/>
<pin name="IOR4"/>
<pin name="IOR5"/>
<pin name="IOR6"/>
<pin name="IOR7"/>
<pin name="IOR8"/>
<pin name="IOR9"/>
<pin name="IOR10"/>
</symbol>
<symbol name="ST11">
<pin name="IOS1"/>
<pin name="IOS2"/>
<pin name="IOS3"/>
<pin name="IOS4"/>
<pin name="IOS5"/>
<pin name="IOS6"/>
<pin name="IOS7"/>
<pin name="IOS8"/>
<pin name="IOS9"/>
<pin name="IOS10"/>
<pin name="IOS11"/>
<pin name="IOT1"/>
<pin name="IOT2"/>
<pin name="IOT3"/>
<pin name="IOT4"/>
<pin name="IOT5"/>
<pin name="IOT6"/>
<pin name="IOT7"/>
<pin name="IOT8"/>
<pin name="IOT9"/>
<pin name="IOT10"/>
<pin name="IOT11"/>
</symbol>
<symbol name="UV11">
<pin name="IOU1"/>
<pin name="IOU2"/>
<pin name="IOU3"/>
<pin name="IOU4"/>
<pin name="IOU5"/>
<pin name="IOU6"/>
<pin name="IOU7"/>
<pin name="IOU8"/>
<pin name="IOU9"/>
<pin name="IOU10"/>
<pin name="IOV1"/>
<pin name="IOV2"/>
<pin name="IOV3"/>
<pin name="IOV4"/>
<pin name="IOV5"/>
<pin name="IOV6"/>
<pin name="IOV7"/>
<pin name="IOV8"/>
<pin name="IOV9"/>
<pin name="IOV10"/>
<pin name="IOV11"/>
</symbol>
<symbol name="X10-599">
<pin name="IOX1"/>
<pin name="IOX2"/>
<pin name="IOX3"/>
<pin name="IOX4"/>
<pin name="IOX5"/>
<pin name="IOX6"/>
<pin name="IOX7"/>
<pin name="IOX8"/>
<pin name="IOX9"/>
<pin name="IOX10"/>
</symbol>
<symbol name="200P599C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="A11-599">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
</symbol>
<symbol name="B11-599">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
</symbol>
<symbol name="C10-599">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
</symbol>
<symbol name="D11-599">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
</symbol>
<symbol name="E11-599">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
</symbol>
<symbol name="F10-599">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
</symbol>
<symbol name="G11-599">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
</symbol>
<symbol name="H11-599">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
</symbol>
<symbol name="I11-599">
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI8"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI11"/>
</symbol>
<symbol name="J12-599">
<pin name="IOJ1"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="IOJ12"/>
</symbol>
<symbol name="K11-599">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
</symbol>
<symbol name="L10-599">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
</symbol>
<symbol name="M11-599">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM4"/>
<pin name="IOM5"/>
<pin name="IOM6"/>
<pin name="IOM7"/>
<pin name="IOM8"/>
<pin name="IOM9"/>
<pin name="IOM10"/>
<pin name="IOM11"/>
</symbol>
<symbol name="N11-599">
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="ION5"/>
<pin name="ION6"/>
<pin name="ION7"/>
<pin name="ION8"/>
<pin name="ION9"/>
<pin name="ION10"/>
<pin name="ION11"/>
</symbol>
<symbol name="O10-599">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOO5"/>
<pin name="IOO6"/>
<pin name="IOO7"/>
<pin name="IOO8"/>
<pin name="IOO9"/>
<pin name="IOO10"/>
</symbol>
<symbol name="P11-599">
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
<pin name="IOP6"/>
<pin name="IOP7"/>
<pin name="IOP8"/>
<pin name="IOP9"/>
<pin name="IOP10"/>
<pin name="IOP11"/>
</symbol>
<symbol name="Q11-599">
<pin name="IOQ1"/>
<pin name="IOQ2"/>
<pin name="IOQ3"/>
<pin name="IOQ4"/>
<pin name="IOQ5"/>
<pin name="IOQ6"/>
<pin name="IOQ7"/>
<pin name="IOQ8"/>
<pin name="IOQ9"/>
<pin name="IOQ10"/>
<pin name="IOQ11"/>
</symbol>
<symbol name="U10-599">
<pin name="IOU1"/>
<pin name="IOU2"/>
<pin name="IOU3"/>
<pin name="IOU4"/>
<pin name="IOU5"/>
<pin name="IOU6"/>
<pin name="IOU7"/>
<pin name="IOU8"/>
<pin name="IOU9"/>
<pin name="IOU10"/>
</symbol>
<symbol name="R10-599">
<pin name="IOR1"/>
<pin name="IOR2"/>
<pin name="IOR3"/>
<pin name="IOR4"/>
<pin name="IOR5"/>
<pin name="IOR6"/>
<pin name="IOR7"/>
<pin name="IOR8"/>
<pin name="IOR9"/>
<pin name="IOR10"/>
</symbol>
<symbol name="S11-599">
<pin name="IOS1"/>
<pin name="IOS2"/>
<pin name="IOS3"/>
<pin name="IOS4"/>
<pin name="IOS5"/>
<pin name="IOS6"/>
<pin name="IOS7"/>
<pin name="IOS8"/>
<pin name="IOS9"/>
<pin name="IOS10"/>
<pin name="IOS11"/>
</symbol>
<symbol name="T11-599">
<pin name="IOT1"/>
<pin name="IOT2"/>
<pin name="IOT3"/>
<pin name="IOT4"/>
<pin name="IOT5"/>
<pin name="IOT6"/>
<pin name="IOT7"/>
<pin name="IOT8"/>
<pin name="IOT9"/>
<pin name="IOT10"/>
<pin name="IOT11"/>
</symbol>
<symbol name="V11-599">
<pin name="IOV1"/>
<pin name="IOV2"/>
<pin name="IOV3"/>
<pin name="IOV4"/>
<pin name="IOV5"/>
<pin name="IOV6"/>
<pin name="IOV7"/>
<pin name="IOV8"/>
<pin name="IOV9"/>
<pin name="IOV10"/>
<pin name="IOV11"/>
</symbol>
<symbol name="W11-599">
<pin name="IOW1"/>
<pin name="IOW2"/>
<pin name="IOW3"/>
<pin name="IOW4"/>
<pin name="IOW5"/>
<pin name="IOW6"/>
<pin name="IOW7"/>
<pin name="IOW8"/>
<pin name="IOW9"/>
<pin name="IOW10"/>
<pin name="IOW11"/>
</symbol>
<symbol name="R240C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="A4-D4">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
</symbol>
<symbol name="E2-J4">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
</symbol>
<symbol name="K4-O3">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
</symbol>
<symbol name="P3-T3">
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOQ1"/>
<pin name="IOQ2"/>
<pin name="IOQ3"/>
<pin name="IOR1"/>
<pin name="IOR2"/>
<pin name="IOS1"/>
<pin name="IOS2"/>
<pin name="IOS3"/>
<pin name="IOT1"/>
<pin name="IOT2"/>
<pin name="IOT3"/>
</symbol>
<symbol name="U4-X4">
<pin name="IOU1"/>
<pin name="IOU2"/>
<pin name="IOU3"/>
<pin name="IOU4"/>
<pin name="IOV1"/>
<pin name="IOV2"/>
<pin name="IOV3"/>
<pin name="IOV4"/>
<pin name="IOW1"/>
<pin name="IOW2"/>
<pin name="IOW3"/>
<pin name="IOX1"/>
<pin name="IOX2"/>
<pin name="IOX3"/>
<pin name="IOX4"/>
</symbol>
<symbol name="122-200">
<pin name="IO11"/>
<pin name="IO21"/>
<pin name="IO31"/>
<pin name="IO41"/>
<pin name="IO51"/>
<pin name="IO61"/>
<pin name="IO71"/>
<pin name="IO81"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO121"/>
<pin name="IO122"/>
</symbol>
<symbol name="201-200">
<pin name="IO123"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO201"/>
</symbol>
<symbol name="261-200">
<pin name="IO202"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO261"/>
</symbol>
<symbol name="351-200">
<pin name="IO262"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO281"/>
<pin name="IO291"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO351"/>
</symbol>
<symbol name="441-200">
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
<pin name="IO371"/>
<pin name="IO381"/>
<pin name="IO382"/>
<pin name="IO391"/>
<pin name="IO401"/>
<pin name="IO411"/>
<pin name="IO412"/>
<pin name="IO421"/>
<pin name="IO422"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO441"/>
</symbol>
<symbol name="522-200">
<pin name="IO442"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO471"/>
<pin name="IO472"/>
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO521"/>
<pin name="IO522"/>
</symbol>
<symbol name="P13-130E">
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
<pin name="IOP6"/>
<pin name="IOP7"/>
<pin name="IOP8"/>
<pin name="IOP9"/>
<pin name="IOP10"/>
<pin name="IOP11"/>
<pin name="IOP12"/>
<pin name="IOP13"/>
</symbol>
<symbol name="130E672C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="51-130E">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
</symbol>
<symbol name="92-130E">
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO91"/>
<pin name="IO92"/>
</symbol>
<symbol name="133-130E">
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
</symbol>
<symbol name="174-130E">
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO174"/>
</symbol>
<symbol name="221-130E">
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO221"/>
</symbol>
<symbol name="261-130E">
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO224"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO234"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO244"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO254"/>
<pin name="IO261"/>
</symbol>
<symbol name="301-130E">
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO274"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO284"/>
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO294"/>
<pin name="IO301"/>
</symbol>
<symbol name="344-130E">
<pin name="IO302"/>
<pin name="IO303"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO314"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO344"/>
</symbol>
<symbol name="384-130E">
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
<pin name="IO354"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
<pin name="IO364"/>
<pin name="IO371"/>
<pin name="IO372"/>
<pin name="IO373"/>
<pin name="IO374"/>
<pin name="IO381"/>
<pin name="IO382"/>
<pin name="IO383"/>
<pin name="IO384"/>
</symbol>
<symbol name="432-130E">
<pin name="IO391"/>
<pin name="IO392"/>
<pin name="IO393"/>
<pin name="IO394"/>
<pin name="IO401"/>
<pin name="IO402"/>
<pin name="IO403"/>
<pin name="IO411"/>
<pin name="IO412"/>
<pin name="IO413"/>
<pin name="IO414"/>
<pin name="IO421"/>
<pin name="IO422"/>
<pin name="IO423"/>
<pin name="IO431"/>
<pin name="IO432"/>
</symbol>
<symbol name="472-130E">
<pin name="IO433"/>
<pin name="IO434"/>
<pin name="IO441"/>
<pin name="IO442"/>
<pin name="IO443"/>
<pin name="IO444"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO453"/>
<pin name="IO454"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO463"/>
<pin name="IO464"/>
<pin name="IO471"/>
<pin name="IO472"/>
</symbol>
<symbol name="513-130E">
<pin name="IO473"/>
<pin name="IO474"/>
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO483"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO493"/>
<pin name="IO494"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO503"/>
<pin name="IO504"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO513"/>
</symbol>
<symbol name="524-130E">
<pin name="IO514"/>
<pin name="IO521"/>
<pin name="IO522"/>
<pin name="IO523"/>
<pin name="IO524"/>
</symbol>
<symbol name="A14-130E">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOA14"/>
</symbol>
<symbol name="I12-130E">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI8"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI11"/>
<pin name="IOI12"/>
</symbol>
<symbol name="M13-130E">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM4"/>
<pin name="IOM5"/>
<pin name="IOM6"/>
<pin name="IOM7"/>
<pin name="IOM8"/>
<pin name="IOM9"/>
<pin name="IOM10"/>
<pin name="IOM11"/>
<pin name="IOM12"/>
<pin name="IOM13"/>
</symbol>
<symbol name="E14-130E">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
</symbol>
<symbol name="B14-130E">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB13"/>
<pin name="IOB14"/>
</symbol>
<symbol name="F13-130E">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
</symbol>
<symbol name="J13-130E">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="IOJ12"/>
<pin name="IOJ13"/>
</symbol>
<symbol name="N13-130E">
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="ION5"/>
<pin name="ION6"/>
<pin name="ION7"/>
<pin name="ION8"/>
<pin name="ION9"/>
<pin name="ION10"/>
<pin name="ION11"/>
<pin name="ION12"/>
<pin name="ION13"/>
</symbol>
<symbol name="C14-130E">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC14"/>
</symbol>
<symbol name="G13-130E">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOG12"/>
<pin name="IOG13"/>
</symbol>
<symbol name="K13-130E">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
<pin name="IOK12"/>
<pin name="IOK13"/>
</symbol>
<symbol name="O13-130E">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOO5"/>
<pin name="IOO6"/>
<pin name="IOO7"/>
<pin name="IOO8"/>
<pin name="IOO9"/>
<pin name="IOO10"/>
<pin name="IOO11"/>
<pin name="IOO12"/>
<pin name="IOO13"/>
</symbol>
<symbol name="D14-130E">
<pin name="IOD1"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
<pin name="IOD14"/>
</symbol>
<symbol name="H13-130E">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
<pin name="IOH12"/>
<pin name="IOH13"/>
</symbol>
<symbol name="L13-130E">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
<pin name="IOL11"/>
<pin name="IOL12"/>
<pin name="IOL13"/>
</symbol>
<symbol name="P16">
<pin name="IOP1"/>
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
<pin name="IOP6"/>
<pin name="IOP7"/>
<pin name="IOP8"/>
<pin name="IOP9"/>
<pin name="IOP10"/>
<pin name="IOP11"/>
<pin name="IOP12"/>
<pin name="IOP13"/>
<pin name="IOP14"/>
<pin name="IOP15"/>
<pin name="IOP16"/>
</symbol>
<symbol name="130V600C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="E16">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
<pin name="IOE15"/>
<pin name="IOE16"/>
</symbol>
<symbol name="I16">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI8"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
<pin name="IOI11"/>
<pin name="IOI12"/>
<pin name="IOI13"/>
<pin name="IOI14"/>
<pin name="IOI15"/>
<pin name="IOI16"/>
</symbol>
<symbol name="M16">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM4"/>
<pin name="IOM5"/>
<pin name="IOM6"/>
<pin name="IOM7"/>
<pin name="IOM8"/>
<pin name="IOM9"/>
<pin name="IOM10"/>
<pin name="IOM11"/>
<pin name="IOM12"/>
<pin name="IOM13"/>
<pin name="IOM14"/>
<pin name="IOM15"/>
<pin name="IOM16"/>
</symbol>
<symbol name="F16">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
<pin name="IOF15"/>
<pin name="IOF16"/>
</symbol>
<symbol name="J16">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="IOJ12"/>
<pin name="IOJ13"/>
<pin name="IOJ14"/>
<pin name="IOJ15"/>
<pin name="IOJ16"/>
</symbol>
<symbol name="N16">
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="ION5"/>
<pin name="ION6"/>
<pin name="ION7"/>
<pin name="ION8"/>
<pin name="ION9"/>
<pin name="ION10"/>
<pin name="ION11"/>
<pin name="ION12"/>
<pin name="ION13"/>
<pin name="ION14"/>
<pin name="ION15"/>
<pin name="ION16"/>
</symbol>
<symbol name="G16">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOG12"/>
<pin name="IOG13"/>
<pin name="IOG14"/>
<pin name="IOG15"/>
<pin name="IOG16"/>
</symbol>
<symbol name="K16">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
<pin name="IOK12"/>
<pin name="IOK13"/>
<pin name="IOK14"/>
<pin name="IOK15"/>
<pin name="IOK16"/>
</symbol>
<symbol name="O16">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOO5"/>
<pin name="IOO6"/>
<pin name="IOO7"/>
<pin name="IOO8"/>
<pin name="IOO9"/>
<pin name="IOO10"/>
<pin name="IOO11"/>
<pin name="IOO12"/>
<pin name="IOO13"/>
<pin name="IOO14"/>
<pin name="IOO15"/>
<pin name="IOO16"/>
</symbol>
<symbol name="D16">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
<pin name="IOD14"/>
<pin name="IOD15"/>
<pin name="IOD16"/>
</symbol>
<symbol name="H16">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
<pin name="IOH12"/>
<pin name="IOH13"/>
<pin name="IOH14"/>
<pin name="IOH15"/>
<pin name="IOH16"/>
</symbol>
<symbol name="L16">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
<pin name="IOL11"/>
<pin name="IOL12"/>
<pin name="IOL13"/>
<pin name="IOL14"/>
<pin name="IOL15"/>
<pin name="IOL16"/>
</symbol>
<symbol name="P12-484">
<pin name="IOP2"/>
<pin name="IOP3"/>
<pin name="IOP4"/>
<pin name="IOP5"/>
<pin name="IOP6"/>
<pin name="IOP7"/>
<pin name="IOP8"/>
<pin name="IOP9"/>
<pin name="IOP10"/>
<pin name="IOP11"/>
<pin name="IOP12"/>
</symbol>
<symbol name="130E484C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="51-484">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
</symbol>
<symbol name="93-484">
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
</symbol>
<symbol name="141-484">
<pin name="IO94"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO141"/>
</symbol>
<symbol name="181-484">
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO174"/>
<pin name="IO181"/>
</symbol>
<symbol name="222-484">
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO222"/>
</symbol>
<symbol name="263-484">
<pin name="IO223"/>
<pin name="IO224"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO234"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO244"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO254"/>
<pin name="IO262"/>
<pin name="IO263"/>
</symbol>
<symbol name="311-484">
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO274"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO284"/>
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO303"/>
<pin name="IO311"/>
</symbol>
<symbol name="354-484">
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO314"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
<pin name="IO354"/>
</symbol>
<symbol name="403-484">
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
<pin name="IO364"/>
<pin name="IO371"/>
<pin name="IO372"/>
<pin name="IO373"/>
<pin name="IO374"/>
<pin name="IO381"/>
<pin name="IO382"/>
<pin name="IO383"/>
<pin name="IO391"/>
<pin name="IO392"/>
<pin name="IO401"/>
<pin name="IO402"/>
<pin name="IO403"/>
</symbol>
<symbol name="451-484">
<pin name="IO411"/>
<pin name="IO412"/>
<pin name="IO413"/>
<pin name="IO414"/>
<pin name="IO421"/>
<pin name="IO422"/>
<pin name="IO423"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO433"/>
<pin name="IO434"/>
<pin name="IO441"/>
<pin name="IO442"/>
<pin name="IO443"/>
<pin name="IO444"/>
<pin name="IO451"/>
</symbol>
<symbol name="493-484">
<pin name="IO452"/>
<pin name="IO453"/>
<pin name="IO454"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO463"/>
<pin name="IO471"/>
<pin name="IO472"/>
<pin name="IO473"/>
<pin name="IO474"/>
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO483"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO493"/>
</symbol>
<symbol name="524-484">
<pin name="IO494"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO503"/>
<pin name="IO504"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO513"/>
<pin name="IO514"/>
<pin name="IO521"/>
<pin name="IO522"/>
<pin name="IO523"/>
<pin name="IO524"/>
</symbol>
<symbol name="A12-484">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
</symbol>
<symbol name="B12-484">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
</symbol>
<symbol name="C12-484">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
</symbol>
<symbol name="D12-484">
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
</symbol>
<symbol name="E11-484">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
</symbol>
<symbol name="F12-484">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
</symbol>
<symbol name="G10-484">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
</symbol>
<symbol name="H10-484">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
</symbol>
<symbol name="I10-484">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI6"/>
<pin name="IOI7"/>
<pin name="IOI8"/>
<pin name="IOI9"/>
<pin name="IOI10"/>
</symbol>
<symbol name="J10-484">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ4"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="IOJ8"/>
<pin name="IOJ9"/>
<pin name="IOJ10"/>
</symbol>
<symbol name="K11-484">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
</symbol>
<symbol name="L10-484">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
</symbol>
<symbol name="M12-484">
<pin name="IOM1"/>
<pin name="IOM2"/>
<pin name="IOM3"/>
<pin name="IOM5"/>
<pin name="IOM6"/>
<pin name="IOM7"/>
<pin name="IOM8"/>
<pin name="IOM9"/>
<pin name="IOM10"/>
<pin name="IOM11"/>
<pin name="IOM12"/>
</symbol>
<symbol name="N11-484">
<pin name="ION1"/>
<pin name="ION2"/>
<pin name="ION3"/>
<pin name="ION4"/>
<pin name="ION5"/>
<pin name="ION6"/>
<pin name="ION7"/>
<pin name="ION8"/>
<pin name="ION9"/>
<pin name="ION10"/>
<pin name="ION11"/>
</symbol>
<symbol name="O12-484">
<pin name="IOO1"/>
<pin name="IOO2"/>
<pin name="IOO3"/>
<pin name="IOO4"/>
<pin name="IOO5"/>
<pin name="IOO6"/>
<pin name="IOO7"/>
<pin name="IOO8"/>
<pin name="IOO9"/>
<pin name="IOO10"/>
<pin name="IOO11"/>
<pin name="IOO12"/>
</symbol>
<symbol name="100B600C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="100P503C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="100R240C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
</symbol>
<symbol name="L11-6">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL11"/>
</symbol>
<symbol name="122-100R">
<pin name="IO11"/>
<pin name="IO21"/>
<pin name="IO31"/>
<pin name="IO41"/>
<pin name="IO51"/>
<pin name="IO61"/>
<pin name="IO71"/>
<pin name="IO81"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
</symbol>
<symbol name="192-100R">
<pin name="IO124"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO164"/>
<pin name="IO171"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO191"/>
<pin name="IO192"/>
</symbol>
<symbol name="261-100R">
<pin name="IO194"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO234"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO261"/>
</symbol>
<symbol name="323-100R">
<pin name="IO263"/>
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO284"/>
<pin name="IO291"/>
<pin name="IO293"/>
<pin name="IO294"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
<pin name="IO321"/>
<pin name="IO323"/>
</symbol>
<symbol name="411-100R">
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
<pin name="IO361"/>
<pin name="IO371"/>
<pin name="IO381"/>
<pin name="IO383"/>
<pin name="IO391"/>
<pin name="IO401"/>
<pin name="IO402"/>
<pin name="IO404"/>
<pin name="IO411"/>
</symbol>
<symbol name="502-100R">
<pin name="IO421"/>
<pin name="IO423"/>
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO441"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO461"/>
<pin name="IO462"/>
<pin name="IO471"/>
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO491"/>
<pin name="IO492"/>
<pin name="IO501"/>
<pin name="IO502"/>
</symbol>
<symbol name="522-100R">
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO521"/>
<pin name="IO522"/>
</symbol>
<symbol name="A10-100R">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
</symbol>
<symbol name="B16-9">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB16"/>
</symbol>
<symbol name="C16-9">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC9"/>
<pin name="IOC11"/>
<pin name="IOC16"/>
</symbol>
<symbol name="D7-7">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
</symbol>
<symbol name="E11-6">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE11"/>
</symbol>
<symbol name="F7-6">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF7"/>
</symbol>
<symbol name="G11-6">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG8"/>
<pin name="IOG11"/>
</symbol>
<symbol name="H8-6">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH8"/>
</symbol>
<symbol name="I12-6">
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI12"/>
</symbol>
<symbol name="J14-6">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ5"/>
<pin name="IOJ13"/>
<pin name="IOJ14"/>
</symbol>
<symbol name="K14-6">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK11"/>
<pin name="IOK14"/>
</symbol>
<symbol name="L11-100">
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL11"/>
</symbol>
<symbol name="A10-10">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
</symbol>
<symbol name="B16-100">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB16"/>
</symbol>
<symbol name="C16-100">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC9"/>
<pin name="IOC11"/>
<pin name="IOC16"/>
</symbol>
<symbol name="D7E11">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE11"/>
</symbol>
<symbol name="F7G11">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF7"/>
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG8"/>
<pin name="IOG11"/>
</symbol>
<symbol name="H8I12">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH8"/>
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOI4"/>
<pin name="IOI5"/>
<pin name="IOI12"/>
</symbol>
<symbol name="J14K14">
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
<pin name="IOJ5"/>
<pin name="IOJ13"/>
<pin name="IOJ14"/>
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK11"/>
<pin name="IOK14"/>
</symbol>
<symbol name="K4L5">
<pin name="IOK1"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
</symbol>
<symbol name="100P208C">
<pin name="/CE" direction="in"/>
<pin name="/CEO" direction="in"/>
<pin name="/CONFIG" direction="in"/>
<pin name="/STATUS" direction="in"/>
<pin name="CONF_DONE" direction="in"/>
<pin name="DATA0" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="GCLK0" direction="in"/>
<pin name="GCLK1" direction="in"/>
<pin name="GND_CKLK" direction="pas"/>
<pin name="IN0" direction="in"/>
<pin name="IN1" direction="in"/>
<pin name="IN2" direction="in"/>
<pin name="IN3" direction="in"/>
<pin name="MSEL0" direction="in"/>
<pin name="MSEL1" direction="in"/>
<pin name="TCK"/>
<pin name="TDI"/>
<pin name="TDO"/>
<pin name="TMS"/>
<pin name="TRST"/>
<pin name="VCC_CKLK" direction="pas"/>
</symbol>
<symbol name="132-208">
<pin name="IO11"/>
<pin name="IO21"/>
<pin name="IO31"/>
<pin name="IO41"/>
<pin name="IO51"/>
<pin name="IO61"/>
<pin name="IO71"/>
<pin name="IO81"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO101"/>
<pin name="IO111"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO131"/>
<pin name="IO132"/>
</symbol>
<symbol name="221-208">
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO201"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO221"/>
</symbol>
<symbol name="311-208">
<pin name="IO222"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO261"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO291"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
</symbol>
<symbol name="421-208">
<pin name="IO321"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO333"/>
<pin name="IO341"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO353"/>
<pin name="IO361"/>
<pin name="IO371"/>
<pin name="IO381"/>
<pin name="IO391"/>
<pin name="IO401"/>
<pin name="IO402"/>
<pin name="IO411"/>
<pin name="IO421"/>
</symbol>
<symbol name="522-208">
<pin name="IO431"/>
<pin name="IO432"/>
<pin name="IO441"/>
<pin name="IO451"/>
<pin name="IO452"/>
<pin name="IO461"/>
<pin name="IO471"/>
<pin name="IO481"/>
<pin name="IO482"/>
<pin name="IO491"/>
<pin name="IO501"/>
<pin name="IO502"/>
<pin name="IO511"/>
<pin name="IO512"/>
<pin name="IO521"/>
<pin name="IO522"/>
</symbol>
<symbol name="A7B7">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
</symbol>
<symbol name="C6D7">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
</symbol>
<symbol name="E4F4G4">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
</symbol>
<symbol name="H5I3J3">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOI1"/>
<pin name="IOI2"/>
<pin name="IOI3"/>
<pin name="IOJ1"/>
<pin name="IOJ2"/>
<pin name="IOJ3"/>
</symbol>
<symbol name="H11">
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
<pin name="IOH8"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
</symbol>
<symbol name="63-40">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
</symbol>
<symbol name="122-40">
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
</symbol>
<symbol name="181-40">
<pin name="IO123"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO141"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO181"/>
</symbol>
<symbol name="232-40">
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO232"/>
</symbol>
<symbol name="292-40">
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
<pin name="IO281"/>
<pin name="IO283"/>
<pin name="IO291"/>
<pin name="IO292"/>
</symbol>
<symbol name="351-40">
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO303"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
</symbol>
<symbol name="363-40">
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
</symbol>
<symbol name="A11">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
</symbol>
<symbol name="E10">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
</symbol>
<symbol name="B10">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
</symbol>
<symbol name="C11_4">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
</symbol>
<symbol name="D11">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
</symbol>
<symbol name="F10">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
</symbol>
<symbol name="G11">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
</symbol>
<symbol name="G7H7">
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOG4"/>
<pin name="IOG5"/>
<pin name="IOG6"/>
<pin name="IOG7"/>
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="IOH4"/>
<pin name="IOH5"/>
<pin name="IOH6"/>
<pin name="IOH7"/>
</symbol>
<symbol name="72-40R">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO72"/>
</symbol>
<symbol name="143-40R">
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
</symbol>
<symbol name="221-40R">
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO181"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO221"/>
</symbol>
<symbol name="291-40R">
<pin name="IO222"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO291"/>
</symbol>
<symbol name="362-40R">
<pin name="IO292"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
</symbol>
<symbol name="A8B7">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
</symbol>
<symbol name="C8D8">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
</symbol>
<symbol name="E8F8">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
</symbol>
<symbol name="F12">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
</symbol>
<symbol name="A12">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
</symbol>
<symbol name="B11">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
</symbol>
<symbol name="C12">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
</symbol>
<symbol name="D12">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
</symbol>
<symbol name="E11">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
</symbol>
<symbol name="F14-30B">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
</symbol>
<symbol name="71-30B">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO71"/>
</symbol>
<symbol name="124-30B">
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO104"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
</symbol>
<symbol name="181-30B">
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO181"/>
</symbol>
<symbol name="231-30B">
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
</symbol>
<symbol name="284-30B">
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO284"/>
</symbol>
<symbol name="351-30B">
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO303"/>
<pin name="IO311"/>
<pin name="IO313"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
</symbol>
<symbol name="363-30B">
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
</symbol>
<symbol name="A16-30B">
<pin name="IOA1"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
</symbol>
<symbol name="B16-30B">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB14"/>
<pin name="IOB16"/>
</symbol>
<symbol name="C16-30B">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC14"/>
<pin name="IOC15"/>
<pin name="IOC16"/>
</symbol>
<symbol name="D16-30B">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD14"/>
<pin name="IOD15"/>
<pin name="IOD16"/>
</symbol>
<symbol name="E16-30B">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE14"/>
<pin name="IOE15"/>
<pin name="IOE16"/>
</symbol>
<symbol name="71-K30EF">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO71"/>
</symbol>
<symbol name="124-K30E">
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
</symbol>
<symbol name="181-K30E">
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO181"/>
</symbol>
<symbol name="231-K30E">
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
</symbol>
<symbol name="281-K30E">
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO264"/>
<pin name="IO271"/>
<pin name="IO273"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
</symbol>
<symbol name="351-K30E">
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
</symbol>
<symbol name="363-K30E">
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
</symbol>
<symbol name="A13">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
</symbol>
<symbol name="B14">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB13"/>
<pin name="IOB14"/>
</symbol>
<symbol name="C14">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC14"/>
</symbol>
<symbol name="D14">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
<pin name="IOD14"/>
</symbol>
<symbol name="E14">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
</symbol>
<symbol name="F14">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
</symbol>
<symbol name="63-K30Q">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
</symbol>
<symbol name="122-K30Q">
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO122"/>
</symbol>
<symbol name="181-K30Q">
<pin name="IO123"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO181"/>
</symbol>
<symbol name="232-K30Q">
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO232"/>
</symbol>
<symbol name="292-K30Q">
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO291"/>
<pin name="IO292"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO253"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO273"/>
</symbol>
<symbol name="351-K30Q">
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO303"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO313"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
</symbol>
<symbol name="363-K30Q">
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
<pin name="IO363"/>
</symbol>
<symbol name="C11">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
</symbol>
<symbol name="72-30E">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO72"/>
</symbol>
<symbol name="143-30E">
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
</symbol>
<symbol name="221-30E">
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO181"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO221"/>
</symbol>
<symbol name="291-30E">
<pin name="IO222"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO252"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO272"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO283"/>
<pin name="IO291"/>
</symbol>
<symbol name="362-30E">
<pin name="IO292"/>
<pin name="IO301"/>
<pin name="IO302"/>
<pin name="IO311"/>
<pin name="IO312"/>
<pin name="IO321"/>
<pin name="IO322"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO362"/>
</symbol>
<symbol name="A9">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
</symbol>
<symbol name="F14-30Q">
<pin name="IOF1"/>
<pin name="IOF3"/>
<pin name="IOF5"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF14"/>
</symbol>
<symbol name="37-30Q">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO73"/>
</symbol>
<symbol name="143-30Q">
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO111"/>
<pin name="IO113"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO131"/>
<pin name="IO133"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
</symbol>
<symbol name="221-30Q">
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO171"/>
<pin name="IO173"/>
<pin name="IO183"/>
<pin name="IO191"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO213"/>
<pin name="IO221"/>
</symbol>
<symbol name="292-30Q">
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO251"/>
<pin name="IO253"/>
<pin name="IO261"/>
<pin name="IO262"/>
<pin name="IO263"/>
<pin name="IO271"/>
<pin name="IO273"/>
<pin name="IO281"/>
<pin name="IO282"/>
<pin name="IO284"/>
<pin name="IO292"/>
</symbol>
<symbol name="363-30Q">
<pin name="IO293"/>
<pin name="IO301"/>
<pin name="IO303"/>
<pin name="IO311"/>
<pin name="IO313"/>
<pin name="IO321"/>
<pin name="IO323"/>
<pin name="IO331"/>
<pin name="IO332"/>
<pin name="IO341"/>
<pin name="IO342"/>
<pin name="IO343"/>
<pin name="IO351"/>
<pin name="IO352"/>
<pin name="IO361"/>
<pin name="IO363"/>
</symbol>
<symbol name="A13-30Q">
<pin name="IOA1"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
</symbol>
<symbol name="D14-30Q">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD10"/>
<pin name="IOD12"/>
<pin name="IOD14"/>
</symbol>
<symbol name="B14-30Q">
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB5"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB14"/>
</symbol>
<symbol name="C14-30Q">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC14"/>
</symbol>
<symbol name="E14-30Q">
<pin name="IOE1"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE10"/>
<pin name="IOE12"/>
<pin name="IOE14"/>
</symbol>
<symbol name="F15">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
<pin name="IOF15"/>
</symbol>
<symbol name="A16-15">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOA14"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
</symbol>
<symbol name="B16-15">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB13"/>
<pin name="IOB14"/>
<pin name="IOB15"/>
</symbol>
<symbol name="C16-14">
<pin name="IOC1"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC14"/>
<pin name="IOC15"/>
<pin name="IOC16"/>
</symbol>
<symbol name="D15-14">
<pin name="IOD1"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
<pin name="IOD14"/>
<pin name="IOD15"/>
</symbol>
<symbol name="E15-14">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
<pin name="IOE15"/>
</symbol>
<symbol name="F11">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
</symbol>
<symbol name="52-20R">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO51"/>
<pin name="IO52"/>
</symbol>
<symbol name="102-20R">
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO101"/>
<pin name="IO102"/>
</symbol>
<symbol name="152-20R">
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
</symbol>
<symbol name="203-20R">
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
</symbol>
<symbol name="244-20R">
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO244"/>
</symbol>
<symbol name="C10">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
</symbol>
<symbol name="244-K10">
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO223"/>
<pin name="IO231"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO241"/>
<pin name="IO242"/>
<pin name="IO243"/>
<pin name="IO244"/>
</symbol>
<symbol name="52-K10">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO51"/>
<pin name="IO52"/>
</symbol>
<symbol name="102-K10">
<pin name="IO53"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO101"/>
<pin name="IO102"/>
</symbol>
<symbol name="151-K10">
<pin name="IO103"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
</symbol>
<symbol name="201-K10">
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO201"/>
</symbol>
<symbol name="7256_208">
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO5"/>
<pin name="IO6"/>
<pin name="IO8"/>
<pin name="IO9"/>
<pin name="IO11"/>
<pin name="IO13"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO27"/>
<pin name="IO29"/>
<pin name="IO30"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO37"/>
<pin name="IO38"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO45"/>
<pin name="IO46"/>
<pin name="IO48"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO53"/>
<pin name="IO54"/>
<pin name="IO56"/>
<pin name="IO57"/>
<pin name="IO59"/>
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO64"/>
<pin name="IO65"/>
<pin name="IO67"/>
<pin name="IO69"/>
<pin name="IO70"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO75"/>
<pin name="IO77-TDI"/>
<pin name="IO78"/>
<pin name="IO80"/>
<pin name="IO81"/>
<pin name="IO83"/>
<pin name="IO85"/>
<pin name="IO86"/>
<pin name="IO88"/>
<pin name="IO89"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO94"/>
<pin name="IO96"/>
<pin name="IO97"/>
<pin name="IO99"/>
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO104"/>
<pin name="IO105"/>
<pin name="IO107"/>
<pin name="IO109-TMS"/>
<pin name="IO110"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO115"/>
<pin name="IO117"/>
<pin name="IO118"/>
<pin name="IO120"/>
<pin name="IO121"/>
<pin name="IO123"/>
<pin name="IO125"/>
<pin name="IO126"/>
<pin name="IO128"/>
<pin name="IO129"/>
<pin name="IO131"/>
<pin name="IO133"/>
<pin name="IO134"/>
<pin name="IO136"/>
<pin name="IO137"/>
<pin name="IO139"/>
<pin name="TDO-IO141"/>
<pin name="IO142"/>
<pin name="IO144"/>
<pin name="IO145"/>
<pin name="IO147"/>
<pin name="IO149"/>
<pin name="IO150"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO155"/>
<pin name="IO157"/>
<pin name="IO158"/>
<pin name="IO160"/>
<pin name="IO161"/>
<pin name="IO163"/>
<pin name="IO165"/>
<pin name="IO166"/>
<pin name="IO168"/>
<pin name="IO169"/>
<pin name="IO171"/>
<pin name="TCK-IO173"/>
<pin name="IO174"/>
<pin name="IO176"/>
<pin name="IO177"/>
<pin name="IO179"/>
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO184"/>
<pin name="IO185"/>
<pin name="IO187"/>
<pin name="IO189"/>
<pin name="IO190"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO195"/>
<pin name="IO197"/>
<pin name="IO198"/>
<pin name="IO200"/>
<pin name="IO201"/>
<pin name="IO203"/>
<pin name="IO205"/>
<pin name="IO206"/>
<pin name="IO208"/>
<pin name="IO209"/>
<pin name="IO211"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO216"/>
<pin name="IO217"/>
<pin name="IO219"/>
<pin name="IO221"/>
<pin name="IO222"/>
<pin name="IO224"/>
<pin name="IO225"/>
<pin name="IO227"/>
<pin name="IO229"/>
<pin name="IO230"/>
<pin name="IO232"/>
<pin name="IO233"/>
<pin name="IO235"/>
<pin name="IO237"/>
<pin name="IO238"/>
<pin name="IO240"/>
<pin name="IO241"/>
<pin name="IO243"/>
<pin name="IO245"/>
<pin name="IO246"/>
<pin name="IO248"/>
<pin name="IO249"/>
<pin name="IO251"/>
<pin name="IO253"/>
<pin name="IO254"/>
<pin name="IO256"/>
</symbol>
<symbol name="7064-T44">
<pin name="IO1"/>
<pin name="IO3"/>
<pin name="IO4"/>
<pin name="IO5"/>
<pin name="IO8/TDI"/>
<pin name="IO11"/>
<pin name="IO14"/>
<pin name="IO16"/>
<pin name="IO17"/>
<pin name="IO19"/>
<pin name="IO20"/>
<pin name="IO21"/>
<pin name="IO24"/>
<pin name="IO25"/>
<pin name="IO30"/>
<pin name="IO32/TMS"/>
<pin name="GCLK1" direction="in"/>
<pin name="GCLR/" direction="in"/>
<pin name="OE1" direction="in"/>
<pin name="OE2-GCLK2" direction="in"/>
<pin name="PD/_VCC" direction="pas"/>
<pin name="IO33"/>
<pin name="IO35"/>
<pin name="IO36"/>
<pin name="IO37"/>
<pin name="IO40"/>
<pin name="IO41"/>
<pin name="IO46"/>
<pin name="IO48/TCK"/>
<pin name="IO49"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO56/TDO"/>
<pin name="IO57"/>
<pin name="IO62"/>
<pin name="IO64"/>
</symbol>
<symbol name="A18">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOA14"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
<pin name="IOA17"/>
<pin name="IOA18"/>
</symbol>
<symbol name="6016CONT">
<pin name="CONF_DONE" direction="in"/>
<pin name="!CE" direction="in"/>
<pin name="!STATUS" direction="in"/>
<pin name="!CONFIG" direction="in"/>
<pin name="DCLK" direction="in"/>
<pin name="MSEL" direction="in"/>
<pin name="DATA0"/>
<pin name="GCLK4"/>
<pin name="GCLK1"/>
<pin name="GCLK2"/>
<pin name="GCLK3"/>
</symbol>
<symbol name="B19">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB13"/>
<pin name="IOB14"/>
<pin name="IOB15"/>
<pin name="IOB16"/>
<pin name="IOB17"/>
<pin name="IOB18"/>
<pin name="IOB19"/>
</symbol>
<symbol name="C18">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC9"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC14"/>
<pin name="IOC15"/>
<pin name="IOC16"/>
<pin name="IOC17"/>
<pin name="IOC18"/>
</symbol>
<symbol name="D18">
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
<pin name="IOD14"/>
<pin name="IOD15"/>
<pin name="IOD16"/>
<pin name="IOD17"/>
<pin name="IOD18"/>
</symbol>
<symbol name="E19">
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE8"/>
<pin name="IOE9"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
<pin name="IOE15"/>
<pin name="IOE16"/>
<pin name="IOE17"/>
<pin name="IOE18"/>
<pin name="IOE19"/>
</symbol>
<symbol name="F19">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF6"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
<pin name="IOF15"/>
<pin name="IOF16"/>
<pin name="IOF17"/>
<pin name="IOF18"/>
<pin name="IOF19"/>
</symbol>
<symbol name="IO11-54">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO33"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO42"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
</symbol>
<symbol name="IO61-94">
<pin name="IO61"/>
<pin name="IO62"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO84"/>
<pin name="IO91"/>
<pin name="IO92"/>
<pin name="IO93"/>
<pin name="IO94"/>
</symbol>
<symbol name="IO101134">
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO103"/>
<pin name="IO104"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO124"/>
<pin name="IO131"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO134"/>
</symbol>
<symbol name="IO141174">
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO144"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
<pin name="IO171"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO174"/>
</symbol>
<symbol name="IO181222">
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO194"/>
<pin name="IO201"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO213"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO222"/>
</symbol>
<symbol name="A15-18">
<pin name="IOA1"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA11"/>
<pin name="IOA12"/>
<pin name="IOA13"/>
<pin name="IOA14"/>
<pin name="IOA15"/>
<pin name="IOA16"/>
<pin name="IOA17"/>
<pin name="IOA18"/>
</symbol>
<symbol name="B16-19">
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOB12"/>
<pin name="IOB14"/>
<pin name="IOB15"/>
<pin name="IOB16"/>
<pin name="IOB17"/>
<pin name="IOB18"/>
</symbol>
<symbol name="C16-18">
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="IOC3"/>
<pin name="IOC4"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="IOC8"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOC12"/>
<pin name="IOC13"/>
<pin name="IOC14"/>
<pin name="IOC16"/>
<pin name="IOC17"/>
<pin name="IOC18"/>
</symbol>
<symbol name="D16-18">
<pin name="IOD1"/>
<pin name="IOD3"/>
<pin name="IOD4"/>
<pin name="IOD5"/>
<pin name="IOD6"/>
<pin name="IOD7"/>
<pin name="IOD8"/>
<pin name="IOD9"/>
<pin name="IOD11"/>
<pin name="IOD12"/>
<pin name="IOD13"/>
<pin name="IOD14"/>
<pin name="IOD15"/>
<pin name="IOD16"/>
<pin name="IOD17"/>
<pin name="IOD18"/>
</symbol>
<symbol name="E16-19">
<pin name="IOE2"/>
<pin name="IOE3"/>
<pin name="IOE4"/>
<pin name="IOE5"/>
<pin name="IOE6"/>
<pin name="IOE7"/>
<pin name="IOE9"/>
<pin name="IOE11"/>
<pin name="IOE12"/>
<pin name="IOE13"/>
<pin name="IOE14"/>
<pin name="IOE15"/>
<pin name="IOE16"/>
<pin name="IOE17"/>
<pin name="IOE18"/>
<pin name="IOE19"/>
</symbol>
<symbol name="F16-19">
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF4"/>
<pin name="IOF5"/>
<pin name="IOF7"/>
<pin name="IOF8"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOF12"/>
<pin name="IOF13"/>
<pin name="IOF14"/>
<pin name="IOF15"/>
<pin name="IOF17"/>
<pin name="IOF18"/>
</symbol>
<symbol name="IO54-2">
<pin name="IO11"/>
<pin name="IO12"/>
<pin name="IO21"/>
<pin name="IO22"/>
<pin name="IO23"/>
<pin name="IO24"/>
<pin name="IO31"/>
<pin name="IO32"/>
<pin name="IO34"/>
<pin name="IO41"/>
<pin name="IO43"/>
<pin name="IO44"/>
<pin name="IO51"/>
<pin name="IO52"/>
<pin name="IO53"/>
<pin name="IO54"/>
</symbol>
<symbol name="IO94-3">
<pin name="IO61"/>
<pin name="IO63"/>
<pin name="IO64"/>
<pin name="IO71"/>
<pin name="IO72"/>
<pin name="IO73"/>
<pin name="IO74"/>
<pin name="IO81"/>
<pin name="IO82"/>
<pin name="IO83"/>
<pin name="IO91"/>
<pin name="IO93"/>
<pin name="IO94"/>
</symbol>
<symbol name="IO134-3">
<pin name="IO101"/>
<pin name="IO102"/>
<pin name="IO104"/>
<pin name="IO111"/>
<pin name="IO112"/>
<pin name="IO113"/>
<pin name="IO114"/>
<pin name="IO121"/>
<pin name="IO122"/>
<pin name="IO123"/>
<pin name="IO132"/>
<pin name="IO133"/>
<pin name="IO134"/>
</symbol>
<symbol name="IO174-2">
<pin name="IO141"/>
<pin name="IO142"/>
<pin name="IO143"/>
<pin name="IO151"/>
<pin name="IO152"/>
<pin name="IO153"/>
<pin name="IO154"/>
<pin name="IO161"/>
<pin name="IO162"/>
<pin name="IO163"/>
<pin name="IO164"/>
<pin name="IO172"/>
<pin name="IO173"/>
<pin name="IO174"/>
</symbol>
<symbol name="IO222-2">
<pin name="IO181"/>
<pin name="IO182"/>
<pin name="IO183"/>
<pin name="IO184"/>
<pin name="IO191"/>
<pin name="IO192"/>
<pin name="IO193"/>
<pin name="IO194"/>
<pin name="IO202"/>
<pin name="IO203"/>
<pin name="IO204"/>
<pin name="IO211"/>
<pin name="IO212"/>
<pin name="IO214"/>
<pin name="IO221"/>
<pin name="IO222"/>
</symbol>
<symbol name="EPM240T100C4">
<pin name="B2/100"/>
<pin name="B1/0"/>
<pin name="B1/1"/>
<pin name="B1/2"/>
<pin name="B1/3"/>
<pin name="B1/4"/>
<pin name="B1/5"/>
<pin name="B1/6"/>
<pin name="VCCIO" direction="pwr"/>
<pin name="GNDIO" direction="pwr"/>
<pin name="GNDINT" direction="pwr"/>
<pin name="B1/10-GCLK0"/>
<pin name="VCCINT" direction="pwr"/>
<pin name="B1/12-GCLK1"/>
<pin name="B1/13"/>
<pin name="B1/14"/>
<pin name="B1/15"/>
<pin name="B1/16"/>
<pin name="B1/17"/>
<pin name="B1/18"/>
<pin name="B1/19"/>
<pin name="B1/20-TMS" direction="in"/>
<pin name="B1/21-TDI" direction="in"/>
<pin name="B1/22-TCK" direction="in"/>
<pin name="B1/24-TDO" direction="out"/>
<pin name="B1/25"/>
<pin name="B1/26"/>
<pin name="B1/27"/>
<pin name="B1/28"/>
<pin name="B1/29"/>
<pin name="VCCIO@1" direction="pwr"/>
<pin name="GNDIO@1" direction="pwr"/>
<pin name="B1/32"/>
<pin name="B1/33"/>
<pin name="B1/34"/>
<pin name="B1/35"/>
<pin name="B1/36"/>
<pin name="B1/37"/>
<pin name="B1/38"/>
<pin name="B1/39"/>
<pin name="B1/40"/>
<pin name="B1/41"/>
<pin name="B1/42-DEV_OE"/>
<pin name="B1/43-DEV_CLRN"/>
<pin name="VCCIO@2" direction="pwr"/>
<pin name="GNDIO@2" direction="pwr"/>
<pin name="B1/46"/>
<pin name="B1/47"/>
<pin name="B1/48"/>
<pin name="B1/49"/>
<pin name="B1/50"/>
<pin name="B2/51"/>
<pin name="B2/52"/>
<pin name="B2/53"/>
<pin name="B2/54"/>
<pin name="B2/55"/>
<pin name="B2/56"/>
<pin name="B2/57"/>
<pin name="VCCIO@3" direction="pwr"/>
<pin name="GNDIO@3" direction="pwr"/>
<pin name="B2/60"/>
<pin name="B2/61-GCLK2"/>
<pin name="VCCINT@1" direction="pwr"/>
<pin name="B2/63-GCLK3"/>
<pin name="GNDINT@1" direction="pwr"/>
<pin name="B2/65"/>
<pin name="B2/66"/>
<pin name="B2/67"/>
<pin name="B2/68"/>
<pin name="B2/69"/>
<pin name="B2/70"/>
<pin name="B2/71"/>
<pin name="B2/72"/>
<pin name="B2/73"/>
<pin name="B2/74"/>
<pin name="B2/75"/>
<pin name="B2/76"/>
<pin name="B2/77"/>
<pin name="GNDIO@4" direction="pwr"/>
<pin name="VCCIO@4" direction="pwr"/>
<pin name="B2/80"/>
<pin name="B2/81"/>
<pin name="B2/82"/>
<pin name="B2/83"/>
<pin name="B2/84"/>
<pin name="B2/85"/>
<pin name="B2/86"/>
<pin name="B2/87"/>
<pin name="B2/88"/>
<pin name="B2/89"/>
<pin name="B2/90"/>
<pin name="B2/91"/>
<pin name="GNDIO@5" direction="pwr"/>
<pin name="VCCIO@5" direction="pwr"/>
<pin name="B2/94"/>
<pin name="B2/95"/>
<pin name="B2/96"/>
<pin name="B2/97"/>
<pin name="B2/98"/>
<pin name="B2/99"/>
</symbol>
<symbol name="EPM240F100">
<pin name="IOC2"/>
<pin name="IOB1"/>
<pin name="IOC1"/>
<pin name="IOD3"/>
<pin name="IOD2"/>
<pin name="IOD1"/>
<pin name="IOE3"/>
<pin name="IOE2"/>
<pin name="IOE1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF1"/>
<pin name="IOG1"/>
<pin name="IOH1"/>
<pin name="IOG2"/>
<pin name="IOG3"/>
<pin name="IOK1"/>
<pin name="IOJ3"/>
<pin name="IOK2"/>
<pin name="IOK3"/>
<pin name="IOH4"/>
<pin name="IOJ4"/>
<pin name="IOK4"/>
<pin name="IOJ5"/>
<pin name="IOK5"/>
<pin name="IOH5"/>
<pin name="IOK6"/>
<pin name="IOH6"/>
<pin name="IOJ6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOJ7"/>
<pin name="IOK9"/>
<pin name="IOH7"/>
<pin name="IOJ8"/>
<pin name="IOH8"/>
<pin name="IOK10"/>
<pin name="IOJ9"/>
<pin name="IOH9"/>
<pin name="IOJ10"/>
<pin name="IOH10"/>
<pin name="IOG8"/>
<pin name="IOG9"/>
<pin name="IOG10"/>
<pin name="IOF10"/>
<pin name="IOF9"/>
<pin name="IOF8"/>
<pin name="IOE10"/>
<pin name="IOE9"/>
<pin name="IOE8"/>
<pin name="IOD10"/>
<pin name="IOC10"/>
<pin name="IOD9"/>
<pin name="IOD8"/>
<pin name="IOB10"/>
<pin name="IOC9"/>
<pin name="IOC8"/>
<pin name="IOB9"/>
<pin name="IOA10"/>
<pin name="IOA9"/>
<pin name="IOB8"/>
<pin name="IOA8"/>
<pin name="IOC7"/>
<pin name="IOB7"/>
<pin name="IOA7"/>
<pin name="IOA6"/>
<pin name="IOB6"/>
<pin name="IOA5"/>
<pin name="IOC6"/>
<pin name="IOB5"/>
<pin name="IOC5"/>
<pin name="IOA4"/>
<pin name="IOB4"/>
<pin name="IOC4"/>
<pin name="IOA3"/>
<pin name="IOA2"/>
<pin name="IOB3"/>
<pin name="IOC3"/>
<pin name="IOA1"/>
<pin name="IOB2"/>
<pin name="TCK" direction="in"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="VCC@7" direction="pwr"/>
<pin name="VCC@8" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
</symbol>
<symbol name="EPM240M100">
<pin name="IOA1"/>
<pin name="IOA2"/>
<pin name="IOA3"/>
<pin name="IOA4"/>
<pin name="IOA5"/>
<pin name="IOA6"/>
<pin name="IOA7"/>
<pin name="IOA8"/>
<pin name="IOA9"/>
<pin name="IOA10"/>
<pin name="IOA11"/>
<pin name="IOB1"/>
<pin name="IOB2"/>
<pin name="IOB3"/>
<pin name="IOB4"/>
<pin name="IOB5"/>
<pin name="IOB6"/>
<pin name="IOB7"/>
<pin name="IOB8"/>
<pin name="IOB9"/>
<pin name="IOB10"/>
<pin name="IOB11"/>
<pin name="IOC1"/>
<pin name="IOC2"/>
<pin name="VCC@8" direction="pwr"/>
<pin name="IOC5"/>
<pin name="IOC6"/>
<pin name="IOC7"/>
<pin name="VCC@7" direction="pwr"/>
<pin name="IOC10"/>
<pin name="IOC11"/>
<pin name="IOD1"/>
<pin name="IOD2"/>
<pin name="IOD3"/>
<pin name="GND@8" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="IOD9"/>
<pin name="IOD10"/>
<pin name="IOD11"/>
<pin name="IOE1"/>
<pin name="IOE2"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="VCC@6" direction="pwr"/>
<pin name="IOE10"/>
<pin name="IOE11"/>
<pin name="IOF1"/>
<pin name="IOF2"/>
<pin name="IOF3"/>
<pin name="IOF9"/>
<pin name="IOF10"/>
<pin name="IOF11"/>
<pin name="IOG1"/>
<pin name="IOG2"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="VCC@5" direction="pwr"/>
<pin name="IOG10"/>
<pin name="IOG11"/>
<pin name="IOH1"/>
<pin name="IOH2"/>
<pin name="IOH3"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="IOH9"/>
<pin name="IOH10"/>
<pin name="IOH11"/>
<pin name="TMS" direction="in"/>
<pin name="TDI" direction="in"/>
<pin name="VCC@3" direction="pwr"/>
<pin name="IOJ5"/>
<pin name="IOJ6"/>
<pin name="IOJ7"/>
<pin name="VCC@4" direction="pwr"/>
<pin name="IOJ10"/>
<pin name="IOJ11"/>
<pin name="TCK" direction="in"/>
<pin name="TDO" direction="out"/>
<pin name="IOK3"/>
<pin name="IOK4"/>
<pin name="IOK5"/>
<pin name="IOK6"/>
<pin name="IOK7"/>
<pin name="IOK8"/>
<pin name="IOK9"/>
<pin name="IOK10"/>
<pin name="IOK11"/>
<pin name="IOL1"/>
<pin name="IOL2"/>
<pin name="IOL3"/>
<pin name="IOL4"/>
<pin name="IOL5"/>
<pin name="IOL6"/>
<pin name="IOL7"/>
<pin name="IOL8"/>
<pin name="IOL9"/>
<pin name="IOL10"/>
<pin name="IOL11"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="EPM7032" prefix="IC">
<description>&lt;b&gt;EPM7032&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="EPM7032"/>
<gate name="P" symbol="PWR3-4"/>
</gates>
<devices>
<device name="J44" package="PLCC44">
<connects>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="GND@1" pad="22"/>
<connect gate="P" pin="GND@2" pad="30"/>
<connect gate="P" pin="GND@3" pad="42"/>
<connect gate="P" pin="VCC" pad="15"/>
<connect gate="P" pin="VCC@1" pad="23"/>
<connect gate="P" pin="VCC@2" pad="35"/>
<connect gate="_" pin="GCLK1" pad="43"/>
<connect gate="_" pin="GCLR/" pad="1"/>
<connect gate="_" pin="IO1" pad="4"/>
<connect gate="_" pin="IO10" pad="14"/>
<connect gate="_" pin="IO11" pad="16"/>
<connect gate="_" pin="IO12" pad="17"/>
<connect gate="_" pin="IO13" pad="18"/>
<connect gate="_" pin="IO14" pad="19"/>
<connect gate="_" pin="IO15" pad="20"/>
<connect gate="_" pin="IO16" pad="21"/>
<connect gate="_" pin="IO17" pad="41"/>
<connect gate="_" pin="IO18" pad="40"/>
<connect gate="_" pin="IO19" pad="39"/>
<connect gate="_" pin="IO2" pad="5"/>
<connect gate="_" pin="IO20/TCK" pad="32"/>
<connect gate="_" pin="IO21" pad="37"/>
<connect gate="_" pin="IO22" pad="36"/>
<connect gate="_" pin="IO23" pad="34"/>
<connect gate="_" pin="IO24" pad="33"/>
<connect gate="_" pin="IO25/TDO" pad="38"/>
<connect gate="_" pin="IO26" pad="31"/>
<connect gate="_" pin="IO27" pad="29"/>
<connect gate="_" pin="IO28" pad="28"/>
<connect gate="_" pin="IO29" pad="27"/>
<connect gate="_" pin="IO3" pad="6"/>
<connect gate="_" pin="IO30" pad="26"/>
<connect gate="_" pin="IO31" pad="25"/>
<connect gate="_" pin="IO32" pad="24"/>
<connect gate="_" pin="IO4/TDI" pad="7"/>
<connect gate="_" pin="IO5" pad="8"/>
<connect gate="_" pin="IO6" pad="9"/>
<connect gate="_" pin="IO7" pad="11"/>
<connect gate="_" pin="IO8" pad="12"/>
<connect gate="_" pin="IO9/TMS" pad="13"/>
<connect gate="_" pin="OE1" pad="44"/>
<connect gate="_" pin="OE2-GCLK2" pad="2"/>
<connect gate="_" pin="PD/_VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S44" package="PLCC-S44">
<connects>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="GND@1" pad="22"/>
<connect gate="P" pin="GND@2" pad="30"/>
<connect gate="P" pin="GND@3" pad="42"/>
<connect gate="P" pin="VCC" pad="15"/>
<connect gate="P" pin="VCC@1" pad="23"/>
<connect gate="P" pin="VCC@2" pad="35"/>
<connect gate="_" pin="GCLK1" pad="43"/>
<connect gate="_" pin="GCLR/" pad="1"/>
<connect gate="_" pin="IO1" pad="4"/>
<connect gate="_" pin="IO10" pad="14"/>
<connect gate="_" pin="IO11" pad="16"/>
<connect gate="_" pin="IO12" pad="17"/>
<connect gate="_" pin="IO13" pad="18"/>
<connect gate="_" pin="IO14" pad="19"/>
<connect gate="_" pin="IO15" pad="20"/>
<connect gate="_" pin="IO16" pad="21"/>
<connect gate="_" pin="IO17" pad="41"/>
<connect gate="_" pin="IO18" pad="40"/>
<connect gate="_" pin="IO19" pad="39"/>
<connect gate="_" pin="IO2" pad="5"/>
<connect gate="_" pin="IO20/TCK" pad="32"/>
<connect gate="_" pin="IO21" pad="37"/>
<connect gate="_" pin="IO22" pad="36"/>
<connect gate="_" pin="IO23" pad="34"/>
<connect gate="_" pin="IO24" pad="33"/>
<connect gate="_" pin="IO25/TDO" pad="38"/>
<connect gate="_" pin="IO26" pad="31"/>
<connect gate="_" pin="IO27" pad="29"/>
<connect gate="_" pin="IO28" pad="28"/>
<connect gate="_" pin="IO29" pad="27"/>
<connect gate="_" pin="IO3" pad="6"/>
<connect gate="_" pin="IO30" pad="26"/>
<connect gate="_" pin="IO31" pad="25"/>
<connect gate="_" pin="IO32" pad="24"/>
<connect gate="_" pin="IO4/TDI" pad="7"/>
<connect gate="_" pin="IO5" pad="8"/>
<connect gate="_" pin="IO6" pad="9"/>
<connect gate="_" pin="IO7" pad="11"/>
<connect gate="_" pin="IO8" pad="12"/>
<connect gate="_" pin="IO9/TMS" pad="13"/>
<connect gate="_" pin="OE1" pad="44"/>
<connect gate="_" pin="OE2-GCLK2" pad="2"/>
<connect gate="_" pin="PD/_VCC" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7032SLC44-6N"/>
<attribute name="OC_FARNELL" value="1549447"/>
<attribute name="OC_NEWARK" value="51R9532"/>
</technology>
</technologies>
</device>
<device name="T44" package="TQFP44">
<connects>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="GND@1" pad="16"/>
<connect gate="P" pin="GND@2" pad="24"/>
<connect gate="P" pin="GND@3" pad="36"/>
<connect gate="P" pin="VCC" pad="9"/>
<connect gate="P" pin="VCC@1" pad="17"/>
<connect gate="P" pin="VCC@2" pad="29"/>
<connect gate="_" pin="GCLK1" pad="37"/>
<connect gate="_" pin="GCLR/" pad="39"/>
<connect gate="_" pin="IO1" pad="42"/>
<connect gate="_" pin="IO10" pad="8"/>
<connect gate="_" pin="IO11" pad="10"/>
<connect gate="_" pin="IO12" pad="11"/>
<connect gate="_" pin="IO13" pad="12"/>
<connect gate="_" pin="IO14" pad="13"/>
<connect gate="_" pin="IO15" pad="14"/>
<connect gate="_" pin="IO16" pad="15"/>
<connect gate="_" pin="IO17" pad="35"/>
<connect gate="_" pin="IO18" pad="34"/>
<connect gate="_" pin="IO19" pad="33"/>
<connect gate="_" pin="IO2" pad="43"/>
<connect gate="_" pin="IO20/TCK" pad="26"/>
<connect gate="_" pin="IO21" pad="31"/>
<connect gate="_" pin="IO22" pad="30"/>
<connect gate="_" pin="IO23" pad="28"/>
<connect gate="_" pin="IO24" pad="27"/>
<connect gate="_" pin="IO25/TDO" pad="32"/>
<connect gate="_" pin="IO26" pad="25"/>
<connect gate="_" pin="IO27" pad="23"/>
<connect gate="_" pin="IO28" pad="22"/>
<connect gate="_" pin="IO29" pad="21"/>
<connect gate="_" pin="IO3" pad="44"/>
<connect gate="_" pin="IO30" pad="20"/>
<connect gate="_" pin="IO31" pad="19"/>
<connect gate="_" pin="IO32" pad="18"/>
<connect gate="_" pin="IO4/TDI" pad="1"/>
<connect gate="_" pin="IO5" pad="2"/>
<connect gate="_" pin="IO6" pad="3"/>
<connect gate="_" pin="IO7" pad="5"/>
<connect gate="_" pin="IO8" pad="6"/>
<connect gate="_" pin="IO9/TMS" pad="7"/>
<connect gate="_" pin="OE1" pad="38"/>
<connect gate="_" pin="OE2-GCLK2" pad="40"/>
<connect gate="_" pin="PD/_VCC" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7032SLC44-6N"/>
<attribute name="OC_FARNELL" value="1549447"/>
<attribute name="OC_NEWARK" value="51R9532"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064" prefix="IC">
<description>&lt;b&gt;EPM7064&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="0" symbol="7064-44"/>
<gate name="P" symbol="PWR3-4"/>
</gates>
<devices>
<device name="J44" package="PLCC44">
<connects>
<connect gate="0" pin="GCLK1" pad="43"/>
<connect gate="0" pin="GCLR/" pad="1"/>
<connect gate="0" pin="IO1" pad="12"/>
<connect gate="0" pin="IO11" pad="6"/>
<connect gate="0" pin="IO14" pad="5"/>
<connect gate="0" pin="IO16" pad="4"/>
<connect gate="0" pin="IO17" pad="21"/>
<connect gate="0" pin="IO19" pad="20"/>
<connect gate="0" pin="IO20" pad="19"/>
<connect gate="0" pin="IO21" pad="18"/>
<connect gate="0" pin="IO24" pad="17"/>
<connect gate="0" pin="IO25" pad="16"/>
<connect gate="0" pin="IO3" pad="11"/>
<connect gate="0" pin="IO30" pad="14"/>
<connect gate="0" pin="IO32/TMS" pad="13"/>
<connect gate="0" pin="IO33" pad="24"/>
<connect gate="0" pin="IO35" pad="25"/>
<connect gate="0" pin="IO36" pad="26"/>
<connect gate="0" pin="IO37" pad="27"/>
<connect gate="0" pin="IO4" pad="9"/>
<connect gate="0" pin="IO40" pad="28"/>
<connect gate="0" pin="IO41" pad="29"/>
<connect gate="0" pin="IO46" pad="31"/>
<connect gate="0" pin="IO48/TCK" pad="32"/>
<connect gate="0" pin="IO49" pad="33"/>
<connect gate="0" pin="IO5" pad="8"/>
<connect gate="0" pin="IO51" pad="34"/>
<connect gate="0" pin="IO52" pad="36"/>
<connect gate="0" pin="IO53" pad="37"/>
<connect gate="0" pin="IO56/TDO" pad="38"/>
<connect gate="0" pin="IO57" pad="39"/>
<connect gate="0" pin="IO62" pad="40"/>
<connect gate="0" pin="IO64" pad="41"/>
<connect gate="0" pin="IO8/TDI" pad="7"/>
<connect gate="0" pin="OE1" pad="44"/>
<connect gate="0" pin="OE2-GCLK2" pad="2"/>
<connect gate="0" pin="PD/_VCC" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="GND@1" pad="22"/>
<connect gate="P" pin="GND@2" pad="30"/>
<connect gate="P" pin="GND@3" pad="42"/>
<connect gate="P" pin="VCC" pad="35"/>
<connect gate="P" pin="VCC@1" pad="23"/>
<connect gate="P" pin="VCC@2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S44" package="PLCC-S44">
<connects>
<connect gate="0" pin="GCLK1" pad="43"/>
<connect gate="0" pin="GCLR/" pad="1"/>
<connect gate="0" pin="IO1" pad="12"/>
<connect gate="0" pin="IO11" pad="6"/>
<connect gate="0" pin="IO14" pad="5"/>
<connect gate="0" pin="IO16" pad="4"/>
<connect gate="0" pin="IO17" pad="21"/>
<connect gate="0" pin="IO19" pad="20"/>
<connect gate="0" pin="IO20" pad="19"/>
<connect gate="0" pin="IO21" pad="18"/>
<connect gate="0" pin="IO24" pad="17"/>
<connect gate="0" pin="IO25" pad="16"/>
<connect gate="0" pin="IO3" pad="11"/>
<connect gate="0" pin="IO30" pad="14"/>
<connect gate="0" pin="IO32/TMS" pad="13"/>
<connect gate="0" pin="IO33" pad="24"/>
<connect gate="0" pin="IO35" pad="25"/>
<connect gate="0" pin="IO36" pad="26"/>
<connect gate="0" pin="IO37" pad="27"/>
<connect gate="0" pin="IO4" pad="9"/>
<connect gate="0" pin="IO40" pad="28"/>
<connect gate="0" pin="IO41" pad="29"/>
<connect gate="0" pin="IO46" pad="31"/>
<connect gate="0" pin="IO48/TCK" pad="32"/>
<connect gate="0" pin="IO49" pad="33"/>
<connect gate="0" pin="IO5" pad="8"/>
<connect gate="0" pin="IO51" pad="34"/>
<connect gate="0" pin="IO52" pad="36"/>
<connect gate="0" pin="IO53" pad="37"/>
<connect gate="0" pin="IO56/TDO" pad="38"/>
<connect gate="0" pin="IO57" pad="39"/>
<connect gate="0" pin="IO62" pad="40"/>
<connect gate="0" pin="IO64" pad="41"/>
<connect gate="0" pin="IO8/TDI" pad="7"/>
<connect gate="0" pin="OE1" pad="44"/>
<connect gate="0" pin="OE2-GCLK2" pad="2"/>
<connect gate="0" pin="PD/_VCC" pad="3"/>
<connect gate="P" pin="GND" pad="10"/>
<connect gate="P" pin="GND@1" pad="22"/>
<connect gate="P" pin="GND@2" pad="30"/>
<connect gate="P" pin="GND@3" pad="42"/>
<connect gate="P" pin="VCC" pad="35"/>
<connect gate="P" pin="VCC@1" pad="23"/>
<connect gate="P" pin="VCC@2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7064SLC44-10N"/>
<attribute name="OC_FARNELL" value="1549449"/>
<attribute name="OC_NEWARK" value="51R0526"/>
</technology>
</technologies>
</device>
<device name="T44" package="TQFP44">
<connects>
<connect gate="0" pin="GCLK1" pad="37"/>
<connect gate="0" pin="GCLR/" pad="39"/>
<connect gate="0" pin="IO1" pad="6"/>
<connect gate="0" pin="IO11" pad="44"/>
<connect gate="0" pin="IO14" pad="43"/>
<connect gate="0" pin="IO16" pad="42"/>
<connect gate="0" pin="IO17" pad="15"/>
<connect gate="0" pin="IO19" pad="14"/>
<connect gate="0" pin="IO20" pad="13"/>
<connect gate="0" pin="IO21" pad="12"/>
<connect gate="0" pin="IO24" pad="11"/>
<connect gate="0" pin="IO25" pad="10"/>
<connect gate="0" pin="IO3" pad="5"/>
<connect gate="0" pin="IO30" pad="8"/>
<connect gate="0" pin="IO32/TMS" pad="7"/>
<connect gate="0" pin="IO33" pad="18"/>
<connect gate="0" pin="IO35" pad="19"/>
<connect gate="0" pin="IO36" pad="20"/>
<connect gate="0" pin="IO37" pad="21"/>
<connect gate="0" pin="IO4" pad="3"/>
<connect gate="0" pin="IO40" pad="22"/>
<connect gate="0" pin="IO41" pad="23"/>
<connect gate="0" pin="IO46" pad="25"/>
<connect gate="0" pin="IO48/TCK" pad="26"/>
<connect gate="0" pin="IO49" pad="27"/>
<connect gate="0" pin="IO5" pad="2"/>
<connect gate="0" pin="IO51" pad="28"/>
<connect gate="0" pin="IO52" pad="30"/>
<connect gate="0" pin="IO53" pad="31"/>
<connect gate="0" pin="IO56/TDO" pad="32"/>
<connect gate="0" pin="IO57" pad="33"/>
<connect gate="0" pin="IO62" pad="34"/>
<connect gate="0" pin="IO64" pad="35"/>
<connect gate="0" pin="IO8/TDI" pad="1"/>
<connect gate="0" pin="OE1" pad="38"/>
<connect gate="0" pin="OE2-GCLK2" pad="40"/>
<connect gate="0" pin="PD/_VCC" pad="9"/>
<connect gate="P" pin="GND" pad="4"/>
<connect gate="P" pin="GND@1" pad="16"/>
<connect gate="P" pin="GND@2" pad="24"/>
<connect gate="P" pin="GND@3" pad="36"/>
<connect gate="P" pin="VCC" pad="17"/>
<connect gate="P" pin="VCC@1" pad="29"/>
<connect gate="P" pin="VCC@2" pad="41"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7064TC44-15"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9653"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064-J68" prefix="IC">
<description>&lt;b&gt;EPM7064&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="P" symbol="PWR8-2-6"/>
<gate name="_" symbol="7064-68"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="GND@1" pad="16"/>
<connect gate="P" pin="GND@2" pad="26"/>
<connect gate="P" pin="GND@3" pad="34"/>
<connect gate="P" pin="GND@4" pad="38"/>
<connect gate="P" pin="GND@5" pad="48"/>
<connect gate="P" pin="GND@6" pad="58"/>
<connect gate="P" pin="GND@7" pad="66"/>
<connect gate="P" pin="VCC" pad="3"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCCIO" pad="11"/>
<connect gate="P" pin="VCCIO@1" pad="21"/>
<connect gate="P" pin="VCCIO@2" pad="31"/>
<connect gate="P" pin="VCCIO@3" pad="43"/>
<connect gate="P" pin="VCCIO@4" pad="53"/>
<connect gate="P" pin="VCCIO@5" pad="63"/>
<connect gate="_" pin="GCLK1" pad="67"/>
<connect gate="_" pin="GCLR/" pad="1"/>
<connect gate="_" pin="IO1" pad="18"/>
<connect gate="_" pin="IO11" pad="9"/>
<connect gate="_" pin="IO12" pad="8"/>
<connect gate="_" pin="IO13" pad="7"/>
<connect gate="_" pin="IO14" pad="5"/>
<connect gate="_" pin="IO16" pad="4"/>
<connect gate="_" pin="IO17" pad="33"/>
<connect gate="_" pin="IO19" pad="32"/>
<connect gate="_" pin="IO20" pad="30"/>
<connect gate="_" pin="IO21" pad="29"/>
<connect gate="_" pin="IO22" pad="28"/>
<connect gate="_" pin="IO24" pad="27"/>
<connect gate="_" pin="IO25" pad="25"/>
<connect gate="_" pin="IO27" pad="24"/>
<connect gate="_" pin="IO28" pad="23"/>
<connect gate="_" pin="IO29" pad="22"/>
<connect gate="_" pin="IO3" pad="17"/>
<connect gate="_" pin="IO30" pad="20"/>
<connect gate="_" pin="IO32/TMS" pad="19"/>
<connect gate="_" pin="IO33" pad="36"/>
<connect gate="_" pin="IO35" pad="37"/>
<connect gate="_" pin="IO36" pad="39"/>
<connect gate="_" pin="IO37" pad="40"/>
<connect gate="_" pin="IO38" pad="41"/>
<connect gate="_" pin="IO4" pad="15"/>
<connect gate="_" pin="IO40" pad="42"/>
<connect gate="_" pin="IO41" pad="44"/>
<connect gate="_" pin="IO43" pad="45"/>
<connect gate="_" pin="IO44" pad="46"/>
<connect gate="_" pin="IO45" pad="47"/>
<connect gate="_" pin="IO46" pad="49"/>
<connect gate="_" pin="IO49" pad="51"/>
<connect gate="_" pin="IO5" pad="14"/>
<connect gate="_" pin="IO51" pad="52"/>
<connect gate="_" pin="IO52" pad="54"/>
<connect gate="_" pin="IO53" pad="55"/>
<connect gate="_" pin="IO54" pad="56"/>
<connect gate="_" pin="IO57" pad="59"/>
<connect gate="_" pin="IO59" pad="60"/>
<connect gate="_" pin="IO6" pad="13"/>
<connect gate="_" pin="IO60" pad="61"/>
<connect gate="_" pin="IO61" pad="62"/>
<connect gate="_" pin="IO62" pad="64"/>
<connect gate="_" pin="IO64" pad="65"/>
<connect gate="_" pin="IO8/TDI" pad="12"/>
<connect gate="_" pin="IO9" pad="10"/>
<connect gate="_" pin="OE1" pad="68"/>
<connect gate="_" pin="OE2-GCLK2" pad="2"/>
<connect gate="_" pin="TCK/IO48" pad="50"/>
<connect gate="_" pin="TDO/IO56" pad="57"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064-J84" prefix="IC">
<description>&lt;b&gt;EPM7064&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="EPM7064S"/>
<gate name="P" symbol="PWR8-2-6"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="GND@1" pad="19"/>
<connect gate="P" pin="GND@2" pad="32"/>
<connect gate="P" pin="GND@3" pad="42"/>
<connect gate="P" pin="GND@4" pad="47"/>
<connect gate="P" pin="GND@5" pad="59"/>
<connect gate="P" pin="GND@6" pad="72"/>
<connect gate="P" pin="GND@7" pad="82"/>
<connect gate="P" pin="VCC" pad="3"/>
<connect gate="P" pin="VCC@1" pad="43"/>
<connect gate="P" pin="VCCIO" pad="13"/>
<connect gate="P" pin="VCCIO@1" pad="26"/>
<connect gate="P" pin="VCCIO@2" pad="38"/>
<connect gate="P" pin="VCCIO@3" pad="53"/>
<connect gate="P" pin="VCCIO@4" pad="66"/>
<connect gate="P" pin="VCCIO@5" pad="78"/>
<connect gate="_" pin="GCLK1" pad="83"/>
<connect gate="_" pin="GCLR/" pad="1"/>
<connect gate="_" pin="IO1" pad="22"/>
<connect gate="_" pin="IO10" pad="11"/>
<connect gate="_" pin="IO11" pad="10"/>
<connect gate="_" pin="IO12" pad="9"/>
<connect gate="_" pin="IO13" pad="8"/>
<connect gate="_" pin="IO14" pad="6"/>
<connect gate="_" pin="IO15" pad="5"/>
<connect gate="_" pin="IO16" pad="4"/>
<connect gate="_" pin="IO17" pad="41"/>
<connect gate="_" pin="IO18" pad="40"/>
<connect gate="_" pin="IO19" pad="39"/>
<connect gate="_" pin="IO2" pad="21"/>
<connect gate="_" pin="IO20" pad="37"/>
<connect gate="_" pin="IO21" pad="36"/>
<connect gate="_" pin="IO22" pad="35"/>
<connect gate="_" pin="IO23" pad="34"/>
<connect gate="_" pin="IO24" pad="33"/>
<connect gate="_" pin="IO25" pad="31"/>
<connect gate="_" pin="IO26" pad="30"/>
<connect gate="_" pin="IO27" pad="29"/>
<connect gate="_" pin="IO28" pad="28"/>
<connect gate="_" pin="IO29" pad="27"/>
<connect gate="_" pin="IO3" pad="20"/>
<connect gate="_" pin="IO30" pad="25"/>
<connect gate="_" pin="IO31" pad="24"/>
<connect gate="_" pin="IO32/TMS" pad="23"/>
<connect gate="_" pin="IO33" pad="44"/>
<connect gate="_" pin="IO34" pad="45"/>
<connect gate="_" pin="IO35" pad="46"/>
<connect gate="_" pin="IO36" pad="48"/>
<connect gate="_" pin="IO37" pad="49"/>
<connect gate="_" pin="IO38" pad="50"/>
<connect gate="_" pin="IO39" pad="51"/>
<connect gate="_" pin="IO4" pad="18"/>
<connect gate="_" pin="IO40" pad="52"/>
<connect gate="_" pin="IO41" pad="54"/>
<connect gate="_" pin="IO42" pad="55"/>
<connect gate="_" pin="IO43" pad="56"/>
<connect gate="_" pin="IO44" pad="57"/>
<connect gate="_" pin="IO45" pad="58"/>
<connect gate="_" pin="IO46" pad="60"/>
<connect gate="_" pin="IO47" pad="61"/>
<connect gate="_" pin="IO49" pad="63"/>
<connect gate="_" pin="IO5" pad="17"/>
<connect gate="_" pin="IO50" pad="64"/>
<connect gate="_" pin="IO51" pad="65"/>
<connect gate="_" pin="IO52" pad="67"/>
<connect gate="_" pin="IO53" pad="68"/>
<connect gate="_" pin="IO54" pad="69"/>
<connect gate="_" pin="IO55" pad="70"/>
<connect gate="_" pin="IO57" pad="73"/>
<connect gate="_" pin="IO58" pad="74"/>
<connect gate="_" pin="IO59" pad="75"/>
<connect gate="_" pin="IO6" pad="16"/>
<connect gate="_" pin="IO60" pad="76"/>
<connect gate="_" pin="IO61" pad="77"/>
<connect gate="_" pin="IO62" pad="79"/>
<connect gate="_" pin="IO63" pad="80"/>
<connect gate="_" pin="IO64" pad="81"/>
<connect gate="_" pin="IO7" pad="15"/>
<connect gate="_" pin="IO8/TDI" pad="14"/>
<connect gate="_" pin="IO9" pad="12"/>
<connect gate="_" pin="OE1" pad="84"/>
<connect gate="_" pin="OE2-GCLK2" pad="2"/>
<connect gate="_" pin="TCK/IO48" pad="62"/>
<connect gate="_" pin="TDO/IO56" pad="71"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7064SLC84-10N"/>
<attribute name="OC_FARNELL" value="1549457"/>
<attribute name="OC_NEWARK" value="51R9623"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064-T100" prefix="IC">
<description>&lt;b&gt;EPM7064&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="EPM7064S"/>
<gate name="P" symbol="PWR8-2-6"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="50"/>
<connect gate="NC11" pin="NC" pad="53"/>
<connect gate="NC12" pin="NC" pad="55"/>
<connect gate="NC13" pin="NC" pad="70"/>
<connect gate="NC14" pin="NC" pad="72"/>
<connect gate="NC15" pin="NC" pad="77"/>
<connect gate="NC16" pin="NC" pad="78"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC3" pin="NC" pad="5"/>
<connect gate="NC4" pin="NC" pad="7"/>
<connect gate="NC5" pin="NC" pad="22"/>
<connect gate="NC6" pin="NC" pad="24"/>
<connect gate="NC7" pin="NC" pad="27"/>
<connect gate="NC8" pin="NC" pad="28"/>
<connect gate="NC9" pin="NC" pad="49"/>
<connect gate="P" pin="GND" pad="38"/>
<connect gate="P" pin="GND@1" pad="86"/>
<connect gate="P" pin="GND@2" pad="11"/>
<connect gate="P" pin="GND@3" pad="26"/>
<connect gate="P" pin="GND@4" pad="43"/>
<connect gate="P" pin="GND@5" pad="59"/>
<connect gate="P" pin="GND@6" pad="74"/>
<connect gate="P" pin="GND@7" pad="95"/>
<connect gate="P" pin="VCC" pad="39"/>
<connect gate="P" pin="VCC@1" pad="91"/>
<connect gate="P" pin="VCCIO" pad="3"/>
<connect gate="P" pin="VCCIO@1" pad="18"/>
<connect gate="P" pin="VCCIO@2" pad="34"/>
<connect gate="P" pin="VCCIO@3" pad="51"/>
<connect gate="P" pin="VCCIO@4" pad="66"/>
<connect gate="P" pin="VCCIO@5" pad="82"/>
<connect gate="_" pin="GCLK1" pad="87"/>
<connect gate="_" pin="GCLR/" pad="89"/>
<connect gate="_" pin="IO1" pad="14"/>
<connect gate="_" pin="IO10" pad="99"/>
<connect gate="_" pin="IO11" pad="98"/>
<connect gate="_" pin="IO12" pad="97"/>
<connect gate="_" pin="IO13" pad="96"/>
<connect gate="_" pin="IO14" pad="94"/>
<connect gate="_" pin="IO15" pad="93"/>
<connect gate="_" pin="IO16" pad="92"/>
<connect gate="_" pin="IO17" pad="37"/>
<connect gate="_" pin="IO18" pad="36"/>
<connect gate="_" pin="IO19" pad="35"/>
<connect gate="_" pin="IO2" pad="13"/>
<connect gate="_" pin="IO20" pad="33"/>
<connect gate="_" pin="IO21" pad="32"/>
<connect gate="_" pin="IO22" pad="31"/>
<connect gate="_" pin="IO23" pad="30"/>
<connect gate="_" pin="IO24" pad="29"/>
<connect gate="_" pin="IO25" pad="25"/>
<connect gate="_" pin="IO26" pad="23"/>
<connect gate="_" pin="IO27" pad="21"/>
<connect gate="_" pin="IO28" pad="20"/>
<connect gate="_" pin="IO29" pad="19"/>
<connect gate="_" pin="IO3" pad="12"/>
<connect gate="_" pin="IO30" pad="17"/>
<connect gate="_" pin="IO31" pad="16"/>
<connect gate="_" pin="IO32/TMS" pad="15"/>
<connect gate="_" pin="IO33" pad="40"/>
<connect gate="_" pin="IO34" pad="41"/>
<connect gate="_" pin="IO35" pad="42"/>
<connect gate="_" pin="IO36" pad="44"/>
<connect gate="_" pin="IO37" pad="45"/>
<connect gate="_" pin="IO38" pad="46"/>
<connect gate="_" pin="IO39" pad="47"/>
<connect gate="_" pin="IO4" pad="10"/>
<connect gate="_" pin="IO40" pad="48"/>
<connect gate="_" pin="IO41" pad="52"/>
<connect gate="_" pin="IO42" pad="54"/>
<connect gate="_" pin="IO43" pad="56"/>
<connect gate="_" pin="IO44" pad="57"/>
<connect gate="_" pin="IO45" pad="58"/>
<connect gate="_" pin="IO46" pad="60"/>
<connect gate="_" pin="IO47" pad="61"/>
<connect gate="_" pin="IO49" pad="63"/>
<connect gate="_" pin="IO5" pad="9"/>
<connect gate="_" pin="IO50" pad="64"/>
<connect gate="_" pin="IO51" pad="65"/>
<connect gate="_" pin="IO52" pad="67"/>
<connect gate="_" pin="IO53" pad="68"/>
<connect gate="_" pin="IO54" pad="69"/>
<connect gate="_" pin="IO55" pad="71"/>
<connect gate="_" pin="IO57" pad="75"/>
<connect gate="_" pin="IO58" pad="76"/>
<connect gate="_" pin="IO59" pad="79"/>
<connect gate="_" pin="IO6" pad="8"/>
<connect gate="_" pin="IO60" pad="80"/>
<connect gate="_" pin="IO61" pad="81"/>
<connect gate="_" pin="IO62" pad="83"/>
<connect gate="_" pin="IO63" pad="84"/>
<connect gate="_" pin="IO64" pad="85"/>
<connect gate="_" pin="IO7" pad="6"/>
<connect gate="_" pin="IO8/TDI" pad="4"/>
<connect gate="_" pin="IO9" pad="100"/>
<connect gate="_" pin="OE1" pad="88"/>
<connect gate="_" pin="OE2-GCLK2" pad="90"/>
<connect gate="_" pin="TCK/IO48" pad="62"/>
<connect gate="_" pin="TDO/IO56" pad="73"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7064STI100-7N"/>
<attribute name="OC_FARNELL" value="1549426"/>
<attribute name="OC_NEWARK" value="51R9650"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7064-P100" prefix="IC">
<description>&lt;b&gt;EPM7064&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="EPM7064S"/>
<gate name="P" symbol="PWR8-2-6"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
</gates>
<devices>
<device name="" package="PQFP100">
<connects>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="52"/>
<connect gate="NC11" pin="NC" pad="55"/>
<connect gate="NC12" pin="NC" pad="57"/>
<connect gate="NC13" pin="NC" pad="72"/>
<connect gate="NC14" pin="NC" pad="74"/>
<connect gate="NC15" pin="NC" pad="79"/>
<connect gate="NC16" pin="NC" pad="80"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC3" pin="NC" pad="7"/>
<connect gate="NC4" pin="NC" pad="9"/>
<connect gate="NC5" pin="NC" pad="24"/>
<connect gate="NC6" pin="NC" pad="26"/>
<connect gate="NC7" pin="NC" pad="29"/>
<connect gate="NC8" pin="NC" pad="30"/>
<connect gate="NC9" pin="NC" pad="51"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="GND@1" pad="28"/>
<connect gate="P" pin="GND@2" pad="40"/>
<connect gate="P" pin="GND@3" pad="45"/>
<connect gate="P" pin="GND@4" pad="61"/>
<connect gate="P" pin="GND@5" pad="76"/>
<connect gate="P" pin="GND@6" pad="88"/>
<connect gate="P" pin="GND@7" pad="97"/>
<connect gate="P" pin="VCC" pad="41"/>
<connect gate="P" pin="VCC@1" pad="93"/>
<connect gate="P" pin="VCCIO" pad="5"/>
<connect gate="P" pin="VCCIO@1" pad="20"/>
<connect gate="P" pin="VCCIO@2" pad="36"/>
<connect gate="P" pin="VCCIO@3" pad="53"/>
<connect gate="P" pin="VCCIO@4" pad="68"/>
<connect gate="P" pin="VCCIO@5" pad="84"/>
<connect gate="_" pin="GCLK1" pad="89"/>
<connect gate="_" pin="GCLR/" pad="91"/>
<connect gate="_" pin="IO1" pad="16"/>
<connect gate="_" pin="IO10" pad="3"/>
<connect gate="_" pin="IO11" pad="100"/>
<connect gate="_" pin="IO12" pad="99"/>
<connect gate="_" pin="IO13" pad="98"/>
<connect gate="_" pin="IO14" pad="96"/>
<connect gate="_" pin="IO15" pad="95"/>
<connect gate="_" pin="IO16" pad="94"/>
<connect gate="_" pin="IO17" pad="39"/>
<connect gate="_" pin="IO18" pad="38"/>
<connect gate="_" pin="IO19" pad="37"/>
<connect gate="_" pin="IO2" pad="15"/>
<connect gate="_" pin="IO20" pad="35"/>
<connect gate="_" pin="IO21" pad="34"/>
<connect gate="_" pin="IO22" pad="33"/>
<connect gate="_" pin="IO23" pad="32"/>
<connect gate="_" pin="IO24" pad="31"/>
<connect gate="_" pin="IO25" pad="27"/>
<connect gate="_" pin="IO26" pad="25"/>
<connect gate="_" pin="IO27" pad="23"/>
<connect gate="_" pin="IO28" pad="22"/>
<connect gate="_" pin="IO29" pad="21"/>
<connect gate="_" pin="IO3" pad="14"/>
<connect gate="_" pin="IO30" pad="19"/>
<connect gate="_" pin="IO31" pad="18"/>
<connect gate="_" pin="IO32/TMS" pad="17"/>
<connect gate="_" pin="IO33" pad="42"/>
<connect gate="_" pin="IO34" pad="43"/>
<connect gate="_" pin="IO35" pad="44"/>
<connect gate="_" pin="IO36" pad="46"/>
<connect gate="_" pin="IO37" pad="47"/>
<connect gate="_" pin="IO38" pad="48"/>
<connect gate="_" pin="IO39" pad="49"/>
<connect gate="_" pin="IO4" pad="12"/>
<connect gate="_" pin="IO40" pad="50"/>
<connect gate="_" pin="IO41" pad="54"/>
<connect gate="_" pin="IO42" pad="56"/>
<connect gate="_" pin="IO43" pad="58"/>
<connect gate="_" pin="IO44" pad="59"/>
<connect gate="_" pin="IO45" pad="60"/>
<connect gate="_" pin="IO46" pad="62"/>
<connect gate="_" pin="IO47" pad="63"/>
<connect gate="_" pin="IO49" pad="65"/>
<connect gate="_" pin="IO5" pad="11"/>
<connect gate="_" pin="IO50" pad="66"/>
<connect gate="_" pin="IO51" pad="67"/>
<connect gate="_" pin="IO52" pad="69"/>
<connect gate="_" pin="IO53" pad="70"/>
<connect gate="_" pin="IO54" pad="71"/>
<connect gate="_" pin="IO55" pad="73"/>
<connect gate="_" pin="IO57" pad="77"/>
<connect gate="_" pin="IO58" pad="78"/>
<connect gate="_" pin="IO59" pad="81"/>
<connect gate="_" pin="IO6" pad="10"/>
<connect gate="_" pin="IO60" pad="82"/>
<connect gate="_" pin="IO61" pad="83"/>
<connect gate="_" pin="IO62" pad="85"/>
<connect gate="_" pin="IO63" pad="86"/>
<connect gate="_" pin="IO64" pad="87"/>
<connect gate="_" pin="IO7" pad="8"/>
<connect gate="_" pin="IO8/TDI" pad="6"/>
<connect gate="_" pin="IO9" pad="4"/>
<connect gate="_" pin="OE1" pad="90"/>
<connect gate="_" pin="OE2-GCLK2" pad="92"/>
<connect gate="_" pin="TCK/IO48" pad="64"/>
<connect gate="_" pin="TDO/IO56" pad="75"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7064STI100-7N"/>
<attribute name="OC_FARNELL" value="1549426"/>
<attribute name="OC_NEWARK" value="51R9650"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7096-J68" prefix="IC">
<description>&lt;b&gt;EPM7064&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7096-68"/>
<gate name="P" symbol="PWR8-2-6"/>
</gates>
<devices>
<device name="" package="PLCC68">
<connects>
<connect gate="P" pin="GND" pad="6"/>
<connect gate="P" pin="GND@1" pad="16"/>
<connect gate="P" pin="GND@2" pad="26"/>
<connect gate="P" pin="GND@3" pad="34"/>
<connect gate="P" pin="GND@4" pad="38"/>
<connect gate="P" pin="GND@5" pad="48"/>
<connect gate="P" pin="GND@6" pad="58"/>
<connect gate="P" pin="GND@7" pad="66"/>
<connect gate="P" pin="VCC" pad="3"/>
<connect gate="P" pin="VCC@1" pad="35"/>
<connect gate="P" pin="VCCIO" pad="11"/>
<connect gate="P" pin="VCCIO@1" pad="21"/>
<connect gate="P" pin="VCCIO@2" pad="31"/>
<connect gate="P" pin="VCCIO@3" pad="43"/>
<connect gate="P" pin="VCCIO@4" pad="53"/>
<connect gate="P" pin="VCCIO@5" pad="63"/>
<connect gate="_" pin="GCLK1" pad="67"/>
<connect gate="_" pin="GCLR/" pad="1"/>
<connect gate="_" pin="IO1" pad="13"/>
<connect gate="_" pin="IO12" pad="7"/>
<connect gate="_" pin="IO14" pad="5"/>
<connect gate="_" pin="IO16" pad="4"/>
<connect gate="_" pin="IO17" pad="23"/>
<connect gate="_" pin="IO19" pad="22"/>
<connect gate="_" pin="IO21" pad="20"/>
<connect gate="_" pin="IO24" pad="19"/>
<connect gate="_" pin="IO25" pad="18"/>
<connect gate="_" pin="IO27" pad="17"/>
<connect gate="_" pin="IO29" pad="15"/>
<connect gate="_" pin="IO32" pad="14"/>
<connect gate="_" pin="IO33" pad="33"/>
<connect gate="_" pin="IO35" pad="32"/>
<connect gate="_" pin="IO37" pad="30"/>
<connect gate="_" pin="IO4" pad="12"/>
<connect gate="_" pin="IO40" pad="29"/>
<connect gate="_" pin="IO41" pad="28"/>
<connect gate="_" pin="IO43" pad="27"/>
<connect gate="_" pin="IO45" pad="25"/>
<connect gate="_" pin="IO48" pad="24"/>
<connect gate="_" pin="IO49" pad="36"/>
<connect gate="_" pin="IO51" pad="37"/>
<connect gate="_" pin="IO53" pad="39"/>
<connect gate="_" pin="IO56" pad="40"/>
<connect gate="_" pin="IO57" pad="41"/>
<connect gate="_" pin="IO59" pad="42"/>
<connect gate="_" pin="IO6" pad="10"/>
<connect gate="_" pin="IO61" pad="44"/>
<connect gate="_" pin="IO64" pad="45"/>
<connect gate="_" pin="IO65" pad="46"/>
<connect gate="_" pin="IO67" pad="47"/>
<connect gate="_" pin="IO69" pad="49"/>
<connect gate="_" pin="IO72" pad="50"/>
<connect gate="_" pin="IO73" pad="51"/>
<connect gate="_" pin="IO75" pad="52"/>
<connect gate="_" pin="IO77" pad="54"/>
<connect gate="_" pin="IO8" pad="9"/>
<connect gate="_" pin="IO80" pad="55"/>
<connect gate="_" pin="IO81" pad="56"/>
<connect gate="_" pin="IO84" pad="57"/>
<connect gate="_" pin="IO86" pad="59"/>
<connect gate="_" pin="IO88" pad="60"/>
<connect gate="_" pin="IO89" pad="61"/>
<connect gate="_" pin="IO9" pad="8"/>
<connect gate="_" pin="IO92" pad="62"/>
<connect gate="_" pin="IO94" pad="64"/>
<connect gate="_" pin="IO96" pad="65"/>
<connect gate="_" pin="OE1" pad="68"/>
<connect gate="_" pin="OE2-GCLK2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7096LC68-10"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9655"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7096-J84" prefix="IC">
<description>&lt;b&gt;EPM7096&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7096-84"/>
<gate name="P" symbol="PWR8-2-6"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="NC1" pin="NC" pad="6"/>
<connect gate="NC2" pin="NC" pad="39"/>
<connect gate="NC3" pin="NC" pad="46"/>
<connect gate="NC4" pin="NC" pad="79"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="GND@1" pad="19"/>
<connect gate="P" pin="GND@2" pad="32"/>
<connect gate="P" pin="GND@3" pad="42"/>
<connect gate="P" pin="GND@4" pad="47"/>
<connect gate="P" pin="GND@5" pad="59"/>
<connect gate="P" pin="GND@6" pad="72"/>
<connect gate="P" pin="GND@7" pad="82"/>
<connect gate="P" pin="VCC" pad="3"/>
<connect gate="P" pin="VCC@1" pad="43"/>
<connect gate="P" pin="VCCIO" pad="13"/>
<connect gate="P" pin="VCCIO@1" pad="26"/>
<connect gate="P" pin="VCCIO@2" pad="38"/>
<connect gate="P" pin="VCCIO@3" pad="53"/>
<connect gate="P" pin="VCCIO@4" pad="66"/>
<connect gate="P" pin="VCCIO@5" pad="78"/>
<connect gate="_" pin="GCLK1" pad="83"/>
<connect gate="_" pin="GCLR/" pad="1"/>
<connect gate="_" pin="IO1" pad="16"/>
<connect gate="_" pin="IO11" pad="9"/>
<connect gate="_" pin="IO12" pad="8"/>
<connect gate="_" pin="IO14" pad="5"/>
<connect gate="_" pin="IO16" pad="4"/>
<connect gate="_" pin="IO17" pad="28"/>
<connect gate="_" pin="IO19" pad="27"/>
<connect gate="_" pin="IO21" pad="25"/>
<connect gate="_" pin="IO22" pad="24"/>
<connect gate="_" pin="IO24" pad="23"/>
<connect gate="_" pin="IO25" pad="22"/>
<connect gate="_" pin="IO27" pad="21"/>
<connect gate="_" pin="IO28" pad="20"/>
<connect gate="_" pin="IO29" pad="18"/>
<connect gate="_" pin="IO3" pad="15"/>
<connect gate="_" pin="IO32" pad="17"/>
<connect gate="_" pin="IO33" pad="41"/>
<connect gate="_" pin="IO35" pad="40"/>
<connect gate="_" pin="IO37" pad="37"/>
<connect gate="_" pin="IO38" pad="36"/>
<connect gate="_" pin="IO4" pad="14"/>
<connect gate="_" pin="IO40" pad="35"/>
<connect gate="_" pin="IO41" pad="34"/>
<connect gate="_" pin="IO43" pad="33"/>
<connect gate="_" pin="IO45" pad="31"/>
<connect gate="_" pin="IO46" pad="30"/>
<connect gate="_" pin="IO48" pad="29"/>
<connect gate="_" pin="IO49" pad="44"/>
<connect gate="_" pin="IO51" pad="45"/>
<connect gate="_" pin="IO53" pad="48"/>
<connect gate="_" pin="IO54" pad="49"/>
<connect gate="_" pin="IO56" pad="50"/>
<connect gate="_" pin="IO57" pad="51"/>
<connect gate="_" pin="IO59" pad="52"/>
<connect gate="_" pin="IO6" pad="12"/>
<connect gate="_" pin="IO61" pad="54"/>
<connect gate="_" pin="IO62" pad="55"/>
<connect gate="_" pin="IO64" pad="56"/>
<connect gate="_" pin="IO65" pad="57"/>
<connect gate="_" pin="IO67" pad="58"/>
<connect gate="_" pin="IO69" pad="60"/>
<connect gate="_" pin="IO70" pad="61"/>
<connect gate="_" pin="IO72" pad="62"/>
<connect gate="_" pin="IO73" pad="63"/>
<connect gate="_" pin="IO75" pad="64"/>
<connect gate="_" pin="IO76" pad="65"/>
<connect gate="_" pin="IO77" pad="67"/>
<connect gate="_" pin="IO8" pad="11"/>
<connect gate="_" pin="IO80" pad="68"/>
<connect gate="_" pin="IO81" pad="69"/>
<connect gate="_" pin="IO83" pad="70"/>
<connect gate="_" pin="IO84" pad="71"/>
<connect gate="_" pin="IO86" pad="73"/>
<connect gate="_" pin="IO88" pad="74"/>
<connect gate="_" pin="IO89" pad="75"/>
<connect gate="_" pin="IO9" pad="10"/>
<connect gate="_" pin="IO91" pad="76"/>
<connect gate="_" pin="IO92" pad="77"/>
<connect gate="_" pin="IO94" pad="80"/>
<connect gate="_" pin="IO96" pad="81"/>
<connect gate="_" pin="OE1" pad="84"/>
<connect gate="_" pin="OE2-GCLK2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7096LC84-10"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9659"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7096-P100" prefix="IC">
<description>&lt;b&gt;EPM7096&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="P" symbol="PWR8-2-6"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="_" symbol="7096"/>
</gates>
<devices>
<device name="" package="PQFP100">
<connects>
<connect gate="NC1" pin="NC" pad="9"/>
<connect gate="NC2" pin="NC" pad="24"/>
<connect gate="NC3" pin="NC" pad="37"/>
<connect gate="NC4" pin="NC" pad="44"/>
<connect gate="NC5" pin="NC" pad="57"/>
<connect gate="NC6" pin="NC" pad="72"/>
<connect gate="NC7" pin="NC" pad="85"/>
<connect gate="NC8" pin="NC" pad="96"/>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="GND@1" pad="28"/>
<connect gate="P" pin="GND@2" pad="40"/>
<connect gate="P" pin="GND@3" pad="45"/>
<connect gate="P" pin="GND@4" pad="61"/>
<connect gate="P" pin="GND@5" pad="76"/>
<connect gate="P" pin="GND@6" pad="88"/>
<connect gate="P" pin="GND@7" pad="97"/>
<connect gate="P" pin="VCC" pad="41"/>
<connect gate="P" pin="VCC@1" pad="93"/>
<connect gate="P" pin="VCCIO" pad="5"/>
<connect gate="P" pin="VCCIO@1" pad="20"/>
<connect gate="P" pin="VCCIO@2" pad="36"/>
<connect gate="P" pin="VCCIO@3" pad="53"/>
<connect gate="P" pin="VCCIO@4" pad="68"/>
<connect gate="P" pin="VCCIO@5" pad="84"/>
<connect gate="_" pin="GCLK1" pad="89"/>
<connect gate="_" pin="GCLR/" pad="91"/>
<connect gate="_" pin="IO1" pad="8"/>
<connect gate="_" pin="IO11" pad="100"/>
<connect gate="_" pin="IO12" pad="99"/>
<connect gate="_" pin="IO13" pad="98"/>
<connect gate="_" pin="IO14" pad="95"/>
<connect gate="_" pin="IO16" pad="94"/>
<connect gate="_" pin="IO17" pad="23"/>
<connect gate="_" pin="IO19" pad="22"/>
<connect gate="_" pin="IO20" pad="21"/>
<connect gate="_" pin="IO21" pad="19"/>
<connect gate="_" pin="IO22" pad="18"/>
<connect gate="_" pin="IO24" pad="17"/>
<connect gate="_" pin="IO25" pad="16"/>
<connect gate="_" pin="IO27" pad="15"/>
<connect gate="_" pin="IO28" pad="14"/>
<connect gate="_" pin="IO29" pad="12"/>
<connect gate="_" pin="IO3" pad="7"/>
<connect gate="_" pin="IO30" pad="11"/>
<connect gate="_" pin="IO32" pad="10"/>
<connect gate="_" pin="IO33" pad="39"/>
<connect gate="_" pin="IO35" pad="38"/>
<connect gate="_" pin="IO36" pad="35"/>
<connect gate="_" pin="IO37" pad="34"/>
<connect gate="_" pin="IO38" pad="33"/>
<connect gate="_" pin="IO4" pad="6"/>
<connect gate="_" pin="IO40" pad="32"/>
<connect gate="_" pin="IO41" pad="31"/>
<connect gate="_" pin="IO43" pad="30"/>
<connect gate="_" pin="IO44" pad="29"/>
<connect gate="_" pin="IO45" pad="27"/>
<connect gate="_" pin="IO46" pad="26"/>
<connect gate="_" pin="IO48" pad="25"/>
<connect gate="_" pin="IO49" pad="42"/>
<connect gate="_" pin="IO5" pad="4"/>
<connect gate="_" pin="IO51" pad="43"/>
<connect gate="_" pin="IO52" pad="46"/>
<connect gate="_" pin="IO53" pad="47"/>
<connect gate="_" pin="IO54" pad="48"/>
<connect gate="_" pin="IO56" pad="49"/>
<connect gate="_" pin="IO57" pad="50"/>
<connect gate="_" pin="IO59" pad="51"/>
<connect gate="_" pin="IO6" pad="3"/>
<connect gate="_" pin="IO60" pad="52"/>
<connect gate="_" pin="IO61" pad="54"/>
<connect gate="_" pin="IO62" pad="55"/>
<connect gate="_" pin="IO64" pad="56"/>
<connect gate="_" pin="IO65" pad="58"/>
<connect gate="_" pin="IO67" pad="59"/>
<connect gate="_" pin="IO68" pad="60"/>
<connect gate="_" pin="IO69" pad="62"/>
<connect gate="_" pin="IO70" pad="63"/>
<connect gate="_" pin="IO72" pad="64"/>
<connect gate="_" pin="IO73" pad="65"/>
<connect gate="_" pin="IO75" pad="66"/>
<connect gate="_" pin="IO76" pad="67"/>
<connect gate="_" pin="IO77" pad="69"/>
<connect gate="_" pin="IO78" pad="70"/>
<connect gate="_" pin="IO8" pad="2"/>
<connect gate="_" pin="IO80" pad="71"/>
<connect gate="_" pin="IO81" pad="73"/>
<connect gate="_" pin="IO83" pad="74"/>
<connect gate="_" pin="IO84" pad="75"/>
<connect gate="_" pin="IO85" pad="77"/>
<connect gate="_" pin="IO86" pad="78"/>
<connect gate="_" pin="IO88" pad="79"/>
<connect gate="_" pin="IO89" pad="80"/>
<connect gate="_" pin="IO9" pad="1"/>
<connect gate="_" pin="IO91" pad="81"/>
<connect gate="_" pin="IO92" pad="82"/>
<connect gate="_" pin="IO93" pad="83"/>
<connect gate="_" pin="IO94" pad="86"/>
<connect gate="_" pin="IO96" pad="87"/>
<connect gate="_" pin="OE1" pad="90"/>
<connect gate="_" pin="OE2-GCLK2" pad="92"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7096QC100-10"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9665"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128-J84" prefix="IC">
<description>&lt;b&gt;EPM70128&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7128-84"/>
<gate name="1" symbol="VCC"/>
<gate name="2" symbol="VCC"/>
<gate name="3" symbol="VCCIO"/>
<gate name="4" symbol="VCCIO"/>
<gate name="5" symbol="VCCIO"/>
<gate name="6" symbol="VCCIO"/>
<gate name="7" symbol="VCCIO"/>
<gate name="8" symbol="VCCIO"/>
<gate name="9" symbol="GND"/>
<gate name="10" symbol="GND"/>
<gate name="11" symbol="GND"/>
<gate name="12" symbol="GND"/>
<gate name="13" symbol="GND"/>
<gate name="14" symbol="GND"/>
<gate name="15" symbol="GND"/>
<gate name="16" symbol="GND"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="1" pin="VCC" pad="3"/>
<connect gate="10" pin="GND" pad="19"/>
<connect gate="11" pin="GND" pad="32"/>
<connect gate="12" pin="GND" pad="47"/>
<connect gate="13" pin="GND" pad="59"/>
<connect gate="14" pin="GND" pad="72"/>
<connect gate="15" pin="GND" pad="42"/>
<connect gate="16" pin="GND" pad="82"/>
<connect gate="2" pin="VCC" pad="43"/>
<connect gate="3" pin="VCCIO" pad="13"/>
<connect gate="4" pin="VCCIO" pad="26"/>
<connect gate="5" pin="VCCIO" pad="38"/>
<connect gate="6" pin="VCCIO" pad="53"/>
<connect gate="7" pin="VCCIO" pad="66"/>
<connect gate="8" pin="VCCIO" pad="78"/>
<connect gate="9" pin="GND" pad="7"/>
<connect gate="_" pin="GCLK1" pad="83"/>
<connect gate="_" pin="GCLR/" pad="1"/>
<connect gate="_" pin="IO101" pad="65"/>
<connect gate="_" pin="IO104" pad="67"/>
<connect gate="_" pin="IO105" pad="68"/>
<connect gate="_" pin="IO107" pad="69"/>
<connect gate="_" pin="IO109" pad="70"/>
<connect gate="_" pin="IO11" pad="8"/>
<connect gate="_" pin="IO115" pad="73"/>
<connect gate="_" pin="IO117" pad="74"/>
<connect gate="_" pin="IO118" pad="75"/>
<connect gate="_" pin="IO120" pad="76"/>
<connect gate="_" pin="IO123" pad="77"/>
<connect gate="_" pin="IO125" pad="79"/>
<connect gate="_" pin="IO126" pad="80"/>
<connect gate="_" pin="IO128" pad="81"/>
<connect gate="_" pin="IO13" pad="6"/>
<connect gate="_" pin="IO14" pad="5"/>
<connect gate="_" pin="IO16" pad="4"/>
<connect gate="_" pin="IO17" pad="22"/>
<connect gate="_" pin="IO19" pad="21"/>
<connect gate="_" pin="IO21" pad="20"/>
<connect gate="_" pin="IO24" pad="18"/>
<connect gate="_" pin="IO25" pad="17"/>
<connect gate="_" pin="IO27" pad="16"/>
<connect gate="_" pin="IO29" pad="15"/>
<connect gate="_" pin="IO3" pad="12"/>
<connect gate="_" pin="IO32/TDI" pad="14"/>
<connect gate="_" pin="IO35" pad="31"/>
<connect gate="_" pin="IO37" pad="30"/>
<connect gate="_" pin="IO38" pad="29"/>
<connect gate="_" pin="IO40" pad="28"/>
<connect gate="_" pin="IO43" pad="27"/>
<connect gate="_" pin="IO45" pad="25"/>
<connect gate="_" pin="IO46" pad="24"/>
<connect gate="_" pin="IO48/TMS" pad="23"/>
<connect gate="_" pin="IO49" pad="41"/>
<connect gate="_" pin="IO5" pad="11"/>
<connect gate="_" pin="IO51" pad="40"/>
<connect gate="_" pin="IO53" pad="39"/>
<connect gate="_" pin="IO56" pad="37"/>
<connect gate="_" pin="IO57" pad="36"/>
<connect gate="_" pin="IO59" pad="35"/>
<connect gate="_" pin="IO6" pad="10"/>
<connect gate="_" pin="IO61" pad="34"/>
<connect gate="_" pin="IO64" pad="33"/>
<connect gate="_" pin="IO65" pad="44"/>
<connect gate="_" pin="IO67" pad="45"/>
<connect gate="_" pin="IO69" pad="46"/>
<connect gate="_" pin="IO72" pad="48"/>
<connect gate="_" pin="IO73" pad="49"/>
<connect gate="_" pin="IO75" pad="50"/>
<connect gate="_" pin="IO77" pad="51"/>
<connect gate="_" pin="IO8" pad="9"/>
<connect gate="_" pin="IO80" pad="52"/>
<connect gate="_" pin="IO83" pad="54"/>
<connect gate="_" pin="IO85" pad="55"/>
<connect gate="_" pin="IO86" pad="56"/>
<connect gate="_" pin="IO88" pad="57"/>
<connect gate="_" pin="IO91" pad="58"/>
<connect gate="_" pin="IO93" pad="60"/>
<connect gate="_" pin="IO94" pad="61"/>
<connect gate="_" pin="IO97" pad="63"/>
<connect gate="_" pin="IO99" pad="64"/>
<connect gate="_" pin="OE1" pad="84"/>
<connect gate="_" pin="OE2-GCLK2" pad="2"/>
<connect gate="_" pin="TCK/IO96" pad="62"/>
<connect gate="_" pin="TDO/IO112" pad="71"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7128SLC84-7N"/>
<attribute name="OC_FARNELL" value="1549458"/>
<attribute name="OC_NEWARK" value="51R9744"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128-?100" prefix="IC">
<description>&lt;b&gt;EPM70128&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7128P100"/>
<gate name="1" symbol="VCC"/>
<gate name="2" symbol="VCC"/>
<gate name="3" symbol="VCCIO"/>
<gate name="4" symbol="VCCIO"/>
<gate name="5" symbol="VCCIO"/>
<gate name="6" symbol="VCCIO"/>
<gate name="7" symbol="VCCIO"/>
<gate name="8" symbol="VCCIO"/>
<gate name="9" symbol="GND"/>
<gate name="10" symbol="GND"/>
<gate name="11" symbol="GND"/>
<gate name="12" symbol="GND"/>
<gate name="13" symbol="GND"/>
<gate name="14" symbol="GND"/>
<gate name="15" symbol="GND"/>
<gate name="16" symbol="GND"/>
</gates>
<devices>
<device name="P" package="PQFP100">
<connects>
<connect gate="1" pin="VCC" pad="41"/>
<connect gate="10" pin="GND" pad="28"/>
<connect gate="11" pin="GND" pad="45"/>
<connect gate="12" pin="GND" pad="61"/>
<connect gate="13" pin="GND" pad="76"/>
<connect gate="14" pin="GND" pad="97"/>
<connect gate="15" pin="GND" pad="40"/>
<connect gate="16" pin="GND" pad="88"/>
<connect gate="2" pin="VCC" pad="93"/>
<connect gate="3" pin="VCCIO" pad="5"/>
<connect gate="4" pin="VCCIO" pad="20"/>
<connect gate="5" pin="VCCIO" pad="36"/>
<connect gate="6" pin="VCCIO" pad="53"/>
<connect gate="7" pin="VCCIO" pad="68"/>
<connect gate="8" pin="VCCIO" pad="84"/>
<connect gate="9" pin="GND" pad="13"/>
<connect gate="_" pin="GCLK1" pad="89"/>
<connect gate="_" pin="GCLR/" pad="91"/>
<connect gate="_" pin="IO1" pad="4"/>
<connect gate="_" pin="IO101" pad="67"/>
<connect gate="_" pin="IO102" pad="69"/>
<connect gate="_" pin="IO104" pad="70"/>
<connect gate="_" pin="IO105" pad="71"/>
<connect gate="_" pin="IO107" pad="72"/>
<connect gate="_" pin="IO109" pad="73"/>
<connect gate="_" pin="IO11" pad="98"/>
<connect gate="_" pin="IO110" pad="74"/>
<connect gate="_" pin="IO113" pad="77"/>
<connect gate="_" pin="IO115" pad="78"/>
<connect gate="_" pin="IO117" pad="79"/>
<connect gate="_" pin="IO118" pad="80"/>
<connect gate="_" pin="IO120" pad="81"/>
<connect gate="_" pin="IO121" pad="82"/>
<connect gate="_" pin="IO123" pad="83"/>
<connect gate="_" pin="IO125" pad="85"/>
<connect gate="_" pin="IO126" pad="86"/>
<connect gate="_" pin="IO128" pad="87"/>
<connect gate="_" pin="IO13" pad="96"/>
<connect gate="_" pin="IO14" pad="95"/>
<connect gate="_" pin="IO16" pad="94"/>
<connect gate="_" pin="IO17" pad="16"/>
<connect gate="_" pin="IO19" pad="15"/>
<connect gate="_" pin="IO21" pad="14"/>
<connect gate="_" pin="IO22" pad="12"/>
<connect gate="_" pin="IO24" pad="11"/>
<connect gate="_" pin="IO25" pad="10"/>
<connect gate="_" pin="IO27" pad="9"/>
<connect gate="_" pin="IO29" pad="8"/>
<connect gate="_" pin="IO3" pad="3"/>
<connect gate="_" pin="IO30" pad="7"/>
<connect gate="_" pin="IO32/TDI" pad="6"/>
<connect gate="_" pin="IO33" pad="27"/>
<connect gate="_" pin="IO35" pad="26"/>
<connect gate="_" pin="IO37" pad="25"/>
<connect gate="_" pin="IO38" pad="24"/>
<connect gate="_" pin="IO40" pad="23"/>
<connect gate="_" pin="IO41" pad="22"/>
<connect gate="_" pin="IO43" pad="21"/>
<connect gate="_" pin="IO45" pad="19"/>
<connect gate="_" pin="IO46" pad="18"/>
<connect gate="_" pin="IO48/TMS" pad="17"/>
<connect gate="_" pin="IO49" pad="39"/>
<connect gate="_" pin="IO5" pad="2"/>
<connect gate="_" pin="IO51" pad="38"/>
<connect gate="_" pin="IO53" pad="37"/>
<connect gate="_" pin="IO54" pad="35"/>
<connect gate="_" pin="IO56" pad="34"/>
<connect gate="_" pin="IO57" pad="33"/>
<connect gate="_" pin="IO59" pad="32"/>
<connect gate="_" pin="IO6" pad="1"/>
<connect gate="_" pin="IO61" pad="31"/>
<connect gate="_" pin="IO62" pad="30"/>
<connect gate="_" pin="IO64" pad="29"/>
<connect gate="_" pin="IO65" pad="42"/>
<connect gate="_" pin="IO67" pad="43"/>
<connect gate="_" pin="IO69" pad="44"/>
<connect gate="_" pin="IO70" pad="46"/>
<connect gate="_" pin="IO72" pad="47"/>
<connect gate="_" pin="IO73" pad="48"/>
<connect gate="_" pin="IO75" pad="49"/>
<connect gate="_" pin="IO77" pad="50"/>
<connect gate="_" pin="IO78" pad="51"/>
<connect gate="_" pin="IO8" pad="100"/>
<connect gate="_" pin="IO80" pad="52"/>
<connect gate="_" pin="IO81" pad="54"/>
<connect gate="_" pin="IO83" pad="55"/>
<connect gate="_" pin="IO85" pad="56"/>
<connect gate="_" pin="IO86" pad="57"/>
<connect gate="_" pin="IO88" pad="58"/>
<connect gate="_" pin="IO89" pad="59"/>
<connect gate="_" pin="IO9" pad="99"/>
<connect gate="_" pin="IO91" pad="60"/>
<connect gate="_" pin="IO93" pad="62"/>
<connect gate="_" pin="IO94" pad="63"/>
<connect gate="_" pin="IO97" pad="65"/>
<connect gate="_" pin="IO99" pad="66"/>
<connect gate="_" pin="OE1" pad="90"/>
<connect gate="_" pin="OE2-GCLK2" pad="92"/>
<connect gate="_" pin="TCM/IO96" pad="64"/>
<connect gate="_" pin="TDO/IO112" pad="75"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7128SQC100-7N"/>
<attribute name="OC_FARNELL" value="1549424"/>
<attribute name="OC_NEWARK" value="51R0530"/>
</technology>
</technologies>
</device>
<device name="T" package="TQFP100">
<connects>
<connect gate="1" pin="VCC" pad="39"/>
<connect gate="10" pin="GND" pad="26"/>
<connect gate="11" pin="GND" pad="43"/>
<connect gate="12" pin="GND" pad="59"/>
<connect gate="13" pin="GND" pad="74"/>
<connect gate="14" pin="GND" pad="86"/>
<connect gate="15" pin="GND" pad="95"/>
<connect gate="16" pin="GND" pad="38"/>
<connect gate="2" pin="VCC" pad="91"/>
<connect gate="3" pin="VCCIO" pad="3"/>
<connect gate="4" pin="VCCIO" pad="18"/>
<connect gate="5" pin="VCCIO" pad="34"/>
<connect gate="6" pin="VCCIO" pad="51"/>
<connect gate="7" pin="VCCIO" pad="66"/>
<connect gate="8" pin="VCCIO" pad="82"/>
<connect gate="9" pin="GND" pad="11"/>
<connect gate="_" pin="GCLK1" pad="87"/>
<connect gate="_" pin="GCLR/" pad="89"/>
<connect gate="_" pin="IO1" pad="2"/>
<connect gate="_" pin="IO101" pad="65"/>
<connect gate="_" pin="IO102" pad="67"/>
<connect gate="_" pin="IO104" pad="68"/>
<connect gate="_" pin="IO105" pad="69"/>
<connect gate="_" pin="IO107" pad="70"/>
<connect gate="_" pin="IO109" pad="71"/>
<connect gate="_" pin="IO11" pad="96"/>
<connect gate="_" pin="IO110" pad="72"/>
<connect gate="_" pin="IO113" pad="75"/>
<connect gate="_" pin="IO115" pad="76"/>
<connect gate="_" pin="IO117" pad="77"/>
<connect gate="_" pin="IO118" pad="78"/>
<connect gate="_" pin="IO120" pad="79"/>
<connect gate="_" pin="IO121" pad="80"/>
<connect gate="_" pin="IO123" pad="81"/>
<connect gate="_" pin="IO125" pad="83"/>
<connect gate="_" pin="IO126" pad="84"/>
<connect gate="_" pin="IO128" pad="85"/>
<connect gate="_" pin="IO13" pad="94"/>
<connect gate="_" pin="IO14" pad="93"/>
<connect gate="_" pin="IO16" pad="92"/>
<connect gate="_" pin="IO17" pad="14"/>
<connect gate="_" pin="IO19" pad="13"/>
<connect gate="_" pin="IO21" pad="12"/>
<connect gate="_" pin="IO22" pad="10"/>
<connect gate="_" pin="IO24" pad="9"/>
<connect gate="_" pin="IO25" pad="8"/>
<connect gate="_" pin="IO27" pad="7"/>
<connect gate="_" pin="IO29" pad="6"/>
<connect gate="_" pin="IO3" pad="1"/>
<connect gate="_" pin="IO30" pad="5"/>
<connect gate="_" pin="IO32/TDI" pad="4"/>
<connect gate="_" pin="IO33" pad="25"/>
<connect gate="_" pin="IO35" pad="24"/>
<connect gate="_" pin="IO37" pad="23"/>
<connect gate="_" pin="IO38" pad="22"/>
<connect gate="_" pin="IO40" pad="21"/>
<connect gate="_" pin="IO41" pad="20"/>
<connect gate="_" pin="IO43" pad="19"/>
<connect gate="_" pin="IO45" pad="17"/>
<connect gate="_" pin="IO46" pad="16"/>
<connect gate="_" pin="IO48/TMS" pad="15"/>
<connect gate="_" pin="IO49" pad="37"/>
<connect gate="_" pin="IO5" pad="100"/>
<connect gate="_" pin="IO51" pad="36"/>
<connect gate="_" pin="IO53" pad="35"/>
<connect gate="_" pin="IO54" pad="33"/>
<connect gate="_" pin="IO56" pad="32"/>
<connect gate="_" pin="IO57" pad="31"/>
<connect gate="_" pin="IO59" pad="30"/>
<connect gate="_" pin="IO6" pad="99"/>
<connect gate="_" pin="IO61" pad="29"/>
<connect gate="_" pin="IO62" pad="28"/>
<connect gate="_" pin="IO64" pad="27"/>
<connect gate="_" pin="IO65" pad="40"/>
<connect gate="_" pin="IO67" pad="41"/>
<connect gate="_" pin="IO69" pad="42"/>
<connect gate="_" pin="IO70" pad="44"/>
<connect gate="_" pin="IO72" pad="45"/>
<connect gate="_" pin="IO73" pad="46"/>
<connect gate="_" pin="IO75" pad="47"/>
<connect gate="_" pin="IO77" pad="48"/>
<connect gate="_" pin="IO78" pad="49"/>
<connect gate="_" pin="IO8" pad="98"/>
<connect gate="_" pin="IO80" pad="50"/>
<connect gate="_" pin="IO81" pad="52"/>
<connect gate="_" pin="IO83" pad="53"/>
<connect gate="_" pin="IO85" pad="54"/>
<connect gate="_" pin="IO86" pad="55"/>
<connect gate="_" pin="IO88" pad="56"/>
<connect gate="_" pin="IO89" pad="57"/>
<connect gate="_" pin="IO9" pad="97"/>
<connect gate="_" pin="IO91" pad="58"/>
<connect gate="_" pin="IO93" pad="60"/>
<connect gate="_" pin="IO94" pad="61"/>
<connect gate="_" pin="IO97" pad="63"/>
<connect gate="_" pin="IO99" pad="64"/>
<connect gate="_" pin="OE1" pad="88"/>
<connect gate="_" pin="OE2-GCLK2" pad="90"/>
<connect gate="_" pin="TCM/IO96" pad="62"/>
<connect gate="_" pin="TDO/IO112" pad="73"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7128STC100-7N"/>
<attribute name="OC_FARNELL" value="1549427"/>
<attribute name="OC_NEWARK" value="51R9778"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7128-P160" prefix="IC">
<description>&lt;b&gt;EPM70128&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="EPM7128"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC40" symbol="NC"/>
<gate name="NC41" symbol="NC"/>
<gate name="NC42" symbol="NC"/>
<gate name="NC43" symbol="NC"/>
<gate name="NC44" symbol="NC"/>
<gate name="1" symbol="VCC"/>
<gate name="2" symbol="VCC"/>
<gate name="3" symbol="VCCIO"/>
<gate name="4" symbol="VCCIO"/>
<gate name="5" symbol="VCCIO"/>
<gate name="6" symbol="VCCIO"/>
<gate name="7" symbol="VCCIO"/>
<gate name="8" symbol="VCCIO"/>
<gate name="9" symbol="GND"/>
<gate name="10" symbol="GND"/>
<gate name="11" symbol="GND"/>
<gate name="12" symbol="GND"/>
<gate name="13" symbol="GND"/>
<gate name="14" symbol="GND"/>
<gate name="15" symbol="GND"/>
<gate name="16" symbol="GND"/>
</gates>
<devices>
<device name="" package="PQFP160">
<connects>
<connect gate="1" pin="VCC" pad="61"/>
<connect gate="10" pin="GND" pad="42"/>
<connect gate="11" pin="GND" pad="60"/>
<connect gate="12" pin="GND" pad="66"/>
<connect gate="13" pin="GND" pad="95"/>
<connect gate="14" pin="GND" pad="113"/>
<connect gate="15" pin="GND" pad="148"/>
<connect gate="16" pin="GND" pad="138"/>
<connect gate="2" pin="VCC" pad="143"/>
<connect gate="3" pin="VCCIO" pad="8"/>
<connect gate="4" pin="VCCIO" pad="26"/>
<connect gate="5" pin="VCCIO" pad="55"/>
<connect gate="6" pin="VCCIO" pad="79"/>
<connect gate="7" pin="VCCIO" pad="104"/>
<connect gate="8" pin="VCCIO" pad="133"/>
<connect gate="9" pin="GND" pad="17"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="36"/>
<connect gate="NC11" pin="NC" pad="37"/>
<connect gate="NC12" pin="NC" pad="38"/>
<connect gate="NC13" pin="NC" pad="39"/>
<connect gate="NC14" pin="NC" pad="40"/>
<connect gate="NC15" pin="NC" pad="44"/>
<connect gate="NC16" pin="NC" pad="45"/>
<connect gate="NC17" pin="NC" pad="46"/>
<connect gate="NC18" pin="NC" pad="47"/>
<connect gate="NC19" pin="NC" pad="74"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC20" pin="NC" pad="75"/>
<connect gate="NC21" pin="NC" pad="76"/>
<connect gate="NC22" pin="NC" pad="77"/>
<connect gate="NC23" pin="NC" pad="81"/>
<connect gate="NC24" pin="NC" pad="82"/>
<connect gate="NC25" pin="NC" pad="83"/>
<connect gate="NC26" pin="NC" pad="84"/>
<connect gate="NC27" pin="NC" pad="85"/>
<connect gate="NC28" pin="NC" pad="86"/>
<connect gate="NC29" pin="NC" pad="87"/>
<connect gate="NC3" pin="NC" pad="3"/>
<connect gate="NC30" pin="NC" pad="114"/>
<connect gate="NC31" pin="NC" pad="115"/>
<connect gate="NC32" pin="NC" pad="116"/>
<connect gate="NC33" pin="NC" pad="117"/>
<connect gate="NC34" pin="NC" pad="118"/>
<connect gate="NC35" pin="NC" pad="119"/>
<connect gate="NC36" pin="NC" pad="120"/>
<connect gate="NC37" pin="NC" pad="124"/>
<connect gate="NC38" pin="NC" pad="125"/>
<connect gate="NC39" pin="NC" pad="126"/>
<connect gate="NC4" pin="NC" pad="4"/>
<connect gate="NC40" pin="NC" pad="127"/>
<connect gate="NC41" pin="NC" pad="154"/>
<connect gate="NC42" pin="NC" pad="155"/>
<connect gate="NC43" pin="NC" pad="156"/>
<connect gate="NC44" pin="NC" pad="157"/>
<connect gate="NC5" pin="NC" pad="5"/>
<connect gate="NC6" pin="NC" pad="6"/>
<connect gate="NC7" pin="NC" pad="7"/>
<connect gate="NC8" pin="NC" pad="34"/>
<connect gate="NC9" pin="NC" pad="35"/>
<connect gate="_" pin="GCLK1" pad="139"/>
<connect gate="_" pin="GCLR/" pad="141"/>
<connect gate="_" pin="IO1" pad="160"/>
<connect gate="_" pin="IO100" pad="102"/>
<connect gate="_" pin="IO101" pad="103"/>
<connect gate="_" pin="IO102" pad="105"/>
<connect gate="_" pin="IO104" pad="106"/>
<connect gate="_" pin="IO105" pad="107"/>
<connect gate="_" pin="IO107" pad="108"/>
<connect gate="_" pin="IO108" pad="109"/>
<connect gate="_" pin="IO109" pad="110"/>
<connect gate="_" pin="IO11" pad="149"/>
<connect gate="_" pin="IO110" pad="111"/>
<connect gate="_" pin="IO113" pad="121"/>
<connect gate="_" pin="IO115" pad="122"/>
<connect gate="_" pin="IO116" pad="123"/>
<connect gate="_" pin="IO117" pad="128"/>
<connect gate="_" pin="IO118" pad="129"/>
<connect gate="_" pin="IO12" pad="147"/>
<connect gate="_" pin="IO120" pad="130"/>
<connect gate="_" pin="IO121" pad="131"/>
<connect gate="_" pin="IO123" pad="132"/>
<connect gate="_" pin="IO124" pad="134"/>
<connect gate="_" pin="IO125" pad="135"/>
<connect gate="_" pin="IO126" pad="136"/>
<connect gate="_" pin="IO128" pad="137"/>
<connect gate="_" pin="IO13" pad="146"/>
<connect gate="_" pin="IO14" pad="145"/>
<connect gate="_" pin="IO16" pad="144"/>
<connect gate="_" pin="IO17" pad="21"/>
<connect gate="_" pin="IO19" pad="20"/>
<connect gate="_" pin="IO20" pad="19"/>
<connect gate="_" pin="IO21" pad="18"/>
<connect gate="_" pin="IO22" pad="16"/>
<connect gate="_" pin="IO24" pad="15"/>
<connect gate="_" pin="IO25" pad="14"/>
<connect gate="_" pin="IO27" pad="13"/>
<connect gate="_" pin="IO28" pad="12"/>
<connect gate="_" pin="IO29" pad="11"/>
<connect gate="_" pin="IO3" pad="159"/>
<connect gate="_" pin="IO30" pad="10"/>
<connect gate="_" pin="IO32/TDI" pad="9"/>
<connect gate="_" pin="IO33" pad="41"/>
<connect gate="_" pin="IO35" pad="33"/>
<connect gate="_" pin="IO36" pad="32"/>
<connect gate="_" pin="IO37" pad="31"/>
<connect gate="_" pin="IO38" pad="30"/>
<connect gate="_" pin="IO4" pad="158"/>
<connect gate="_" pin="IO40" pad="29"/>
<connect gate="_" pin="IO41" pad="28"/>
<connect gate="_" pin="IO43" pad="27"/>
<connect gate="_" pin="IO44" pad="25"/>
<connect gate="_" pin="IO45" pad="24"/>
<connect gate="_" pin="IO46" pad="23"/>
<connect gate="_" pin="IO48/TMS" pad="22"/>
<connect gate="_" pin="IO49" pad="59"/>
<connect gate="_" pin="IO5" pad="153"/>
<connect gate="_" pin="IO51" pad="58"/>
<connect gate="_" pin="IO52" pad="57"/>
<connect gate="_" pin="IO53" pad="56"/>
<connect gate="_" pin="IO54" pad="54"/>
<connect gate="_" pin="IO56" pad="53"/>
<connect gate="_" pin="IO57" pad="52"/>
<connect gate="_" pin="IO59" pad="51"/>
<connect gate="_" pin="IO6" pad="152"/>
<connect gate="_" pin="IO60" pad="50"/>
<connect gate="_" pin="IO61" pad="49"/>
<connect gate="_" pin="IO62" pad="48"/>
<connect gate="_" pin="IO64" pad="43"/>
<connect gate="_" pin="IO65" pad="62"/>
<connect gate="_" pin="IO67" pad="63"/>
<connect gate="_" pin="IO68" pad="64"/>
<connect gate="_" pin="IO69" pad="65"/>
<connect gate="_" pin="IO70" pad="67"/>
<connect gate="_" pin="IO72" pad="68"/>
<connect gate="_" pin="IO73" pad="69"/>
<connect gate="_" pin="IO75" pad="70"/>
<connect gate="_" pin="IO76" pad="71"/>
<connect gate="_" pin="IO77" pad="72"/>
<connect gate="_" pin="IO78" pad="73"/>
<connect gate="_" pin="IO8" pad="151"/>
<connect gate="_" pin="IO80" pad="78"/>
<connect gate="_" pin="IO81" pad="80"/>
<connect gate="_" pin="IO83" pad="88"/>
<connect gate="_" pin="IO84" pad="89"/>
<connect gate="_" pin="IO85" pad="90"/>
<connect gate="_" pin="IO86" pad="91"/>
<connect gate="_" pin="IO88" pad="92"/>
<connect gate="_" pin="IO89" pad="93"/>
<connect gate="_" pin="IO9" pad="150"/>
<connect gate="_" pin="IO91" pad="94"/>
<connect gate="_" pin="IO92" pad="96"/>
<connect gate="_" pin="IO93" pad="97"/>
<connect gate="_" pin="IO94" pad="98"/>
<connect gate="_" pin="IO97" pad="100"/>
<connect gate="_" pin="IO99" pad="101"/>
<connect gate="_" pin="OE1" pad="140"/>
<connect gate="_" pin="OE2-GCLK2" pad="142"/>
<connect gate="_" pin="TCK/IO96" pad="99"/>
<connect gate="_" pin="TDO/IO112" pad="112"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7128SQC160-10N"/>
<attribute name="OC_FARNELL" value="1549435"/>
<attribute name="OC_NEWARK" value="51R9760"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7256-RQ208" prefix="IC">
<description>&lt;b&gt;EPM7256E&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7256R208"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
</gates>
<devices>
<device name="" package="RQFP208">
<connects>
<connect gate="G1" pin="GND" pad="14"/>
<connect gate="G10" pin="GND" pad="152"/>
<connect gate="G11" pin="GND" pad="174"/>
<connect gate="G12" pin="GND" pad="180"/>
<connect gate="G13" pin="GND" pad="185"/>
<connect gate="G14" pin="GND" pad="200"/>
<connect gate="G2" pin="GND" pad="32"/>
<connect gate="G3" pin="GND" pad="50"/>
<connect gate="G4" pin="GND" pad="72"/>
<connect gate="G5" pin="GND" pad="75"/>
<connect gate="G6" pin="GND" pad="82"/>
<connect gate="G7" pin="GND" pad="94"/>
<connect gate="G8" pin="GND" pad="116"/>
<connect gate="G9" pin="GND" pad="134"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="106"/>
<connect gate="NC11" pin="NC" pad="155"/>
<connect gate="NC12" pin="NC" pad="156"/>
<connect gate="NC13" pin="NC" pad="157"/>
<connect gate="NC14" pin="NC" pad="158"/>
<connect gate="NC15" pin="NC" pad="207"/>
<connect gate="NC16" pin="NC" pad="208"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC3" pin="NC" pad="51"/>
<connect gate="NC4" pin="NC" pad="52"/>
<connect gate="NC5" pin="NC" pad="53"/>
<connect gate="NC6" pin="NC" pad="54"/>
<connect gate="NC7" pin="NC" pad="103"/>
<connect gate="NC8" pin="NC" pad="104"/>
<connect gate="NC9" pin="NC" pad="105"/>
<connect gate="V1" pin="VCC" pad="74"/>
<connect gate="V2" pin="VCC" pad="83"/>
<connect gate="V3" pin="VCC" pad="179"/>
<connect gate="V4" pin="VCC" pad="186"/>
<connect gate="VO1" pin="VCCIO" pad="5"/>
<connect gate="VO10" pin="VCCIO" pad="191"/>
<connect gate="VO2" pin="VCCIO" pad="23"/>
<connect gate="VO3" pin="VCCIO" pad="41"/>
<connect gate="VO4" pin="VCCIO" pad="63"/>
<connect gate="VO5" pin="VCCIO" pad="85"/>
<connect gate="VO6" pin="VCCIO" pad="107"/>
<connect gate="VO7" pin="VCCIO" pad="125"/>
<connect gate="VO8" pin="VCCIO" pad="143"/>
<connect gate="VO9" pin="VCCIO" pad="165"/>
<connect gate="_" pin="GCLK1" pad="184"/>
<connect gate="_" pin="GCLR/" pad="182"/>
<connect gate="_" pin="IO1" pad="153"/>
<connect gate="_" pin="IO101" pad="121"/>
<connect gate="_" pin="IO102" pad="122"/>
<connect gate="_" pin="IO104" pad="123"/>
<connect gate="_" pin="IO105" pad="124"/>
<connect gate="_" pin="IO107" pad="126"/>
<connect gate="_" pin="IO109-TMS" pad="127"/>
<connect gate="_" pin="IO11" pad="163"/>
<connect gate="_" pin="IO110" pad="128"/>
<connect gate="_" pin="IO112" pad="129"/>
<connect gate="_" pin="IO113" pad="79"/>
<connect gate="_" pin="IO115" pad="80"/>
<connect gate="_" pin="IO117" pad="81"/>
<connect gate="_" pin="IO118" pad="84"/>
<connect gate="_" pin="IO120" pad="86"/>
<connect gate="_" pin="IO121" pad="87"/>
<connect gate="_" pin="IO123" pad="88"/>
<connect gate="_" pin="IO125" pad="89"/>
<connect gate="_" pin="IO126" pad="90"/>
<connect gate="_" pin="IO128" pad="91"/>
<connect gate="_" pin="IO129" pad="197"/>
<connect gate="_" pin="IO13" pad="164"/>
<connect gate="_" pin="IO131" pad="196"/>
<connect gate="_" pin="IO133" pad="195"/>
<connect gate="_" pin="IO134" pad="194"/>
<connect gate="_" pin="IO136" pad="193"/>
<connect gate="_" pin="IO137" pad="192"/>
<connect gate="_" pin="IO139" pad="190"/>
<connect gate="_" pin="IO14" pad="166"/>
<connect gate="_" pin="IO142" pad="188"/>
<connect gate="_" pin="IO144" pad="187"/>
<connect gate="_" pin="IO145" pad="27"/>
<connect gate="_" pin="IO147" pad="26"/>
<connect gate="_" pin="IO149" pad="25"/>
<connect gate="_" pin="IO150" pad="24"/>
<connect gate="_" pin="IO152" pad="22"/>
<connect gate="_" pin="IO153" pad="21"/>
<connect gate="_" pin="IO155" pad="20"/>
<connect gate="_" pin="IO157" pad="19"/>
<connect gate="_" pin="IO158" pad="18"/>
<connect gate="_" pin="IO16" pad="167"/>
<connect gate="_" pin="IO160" pad="17"/>
<connect gate="_" pin="IO161" pad="38"/>
<connect gate="_" pin="IO163" pad="37"/>
<connect gate="_" pin="IO165" pad="36"/>
<connect gate="_" pin="IO166" pad="35"/>
<connect gate="_" pin="IO168" pad="34"/>
<connect gate="_" pin="IO169" pad="33"/>
<connect gate="_" pin="IO17" pad="141"/>
<connect gate="_" pin="IO171" pad="31"/>
<connect gate="_" pin="IO174" pad="29"/>
<connect gate="_" pin="IO176" pad="28"/>
<connect gate="_" pin="IO177" pad="66"/>
<connect gate="_" pin="IO179" pad="67"/>
<connect gate="_" pin="IO181" pad="68"/>
<connect gate="_" pin="IO182" pad="69"/>
<connect gate="_" pin="IO184" pad="70"/>
<connect gate="_" pin="IO185" pad="71"/>
<connect gate="_" pin="IO187" pad="73"/>
<connect gate="_" pin="IO189" pad="76"/>
<connect gate="_" pin="IO19" pad="142"/>
<connect gate="_" pin="IO190" pad="77"/>
<connect gate="_" pin="IO192" pad="78"/>
<connect gate="_" pin="IO193" pad="4"/>
<connect gate="_" pin="IO195" pad="3"/>
<connect gate="_" pin="IO197" pad="206"/>
<connect gate="_" pin="IO198" pad="205"/>
<connect gate="_" pin="IO200" pad="204"/>
<connect gate="_" pin="IO201" pad="203"/>
<connect gate="_" pin="IO203" pad="202"/>
<connect gate="_" pin="IO205" pad="201"/>
<connect gate="_" pin="IO206" pad="199"/>
<connect gate="_" pin="IO208" pad="198"/>
<connect gate="_" pin="IO209" pad="16"/>
<connect gate="_" pin="IO21" pad="144"/>
<connect gate="_" pin="IO211" pad="15"/>
<connect gate="_" pin="IO213" pad="13"/>
<connect gate="_" pin="IO214" pad="12"/>
<connect gate="_" pin="IO216" pad="11"/>
<connect gate="_" pin="IO217" pad="10"/>
<connect gate="_" pin="IO219" pad="9"/>
<connect gate="_" pin="IO22" pad="145"/>
<connect gate="_" pin="IO221" pad="8"/>
<connect gate="_" pin="IO222" pad="7"/>
<connect gate="_" pin="IO224" pad="6"/>
<connect gate="_" pin="IO225" pad="49"/>
<connect gate="_" pin="IO227" pad="48"/>
<connect gate="_" pin="IO229" pad="47"/>
<connect gate="_" pin="IO230" pad="46"/>
<connect gate="_" pin="IO232" pad="45"/>
<connect gate="_" pin="IO233" pad="44"/>
<connect gate="_" pin="IO235" pad="43"/>
<connect gate="_" pin="IO237" pad="42"/>
<connect gate="_" pin="IO238" pad="40"/>
<connect gate="_" pin="IO24" pad="146"/>
<connect gate="_" pin="IO240" pad="39"/>
<connect gate="_" pin="IO241" pad="65"/>
<connect gate="_" pin="IO243" pad="64"/>
<connect gate="_" pin="IO245" pad="62"/>
<connect gate="_" pin="IO246" pad="61"/>
<connect gate="_" pin="IO248" pad="60"/>
<connect gate="_" pin="IO249" pad="59"/>
<connect gate="_" pin="IO25" pad="147"/>
<connect gate="_" pin="IO251" pad="58"/>
<connect gate="_" pin="IO253" pad="57"/>
<connect gate="_" pin="IO254" pad="56"/>
<connect gate="_" pin="IO256" pad="55"/>
<connect gate="_" pin="IO27" pad="148"/>
<connect gate="_" pin="IO29" pad="149"/>
<connect gate="_" pin="IO3" pad="154"/>
<connect gate="_" pin="IO30" pad="150"/>
<connect gate="_" pin="IO32" pad="151"/>
<connect gate="_" pin="IO33" pad="108"/>
<connect gate="_" pin="IO35" pad="109"/>
<connect gate="_" pin="IO37" pad="110"/>
<connect gate="_" pin="IO38" pad="111"/>
<connect gate="_" pin="IO40" pad="112"/>
<connect gate="_" pin="IO41" pad="113"/>
<connect gate="_" pin="IO43" pad="114"/>
<connect gate="_" pin="IO45" pad="115"/>
<connect gate="_" pin="IO46" pad="117"/>
<connect gate="_" pin="IO48" pad="118"/>
<connect gate="_" pin="IO49" pad="92"/>
<connect gate="_" pin="IO5" pad="159"/>
<connect gate="_" pin="IO51" pad="93"/>
<connect gate="_" pin="IO53" pad="95"/>
<connect gate="_" pin="IO54" pad="96"/>
<connect gate="_" pin="IO56" pad="97"/>
<connect gate="_" pin="IO57" pad="98"/>
<connect gate="_" pin="IO59" pad="99"/>
<connect gate="_" pin="IO6" pad="160"/>
<connect gate="_" pin="IO61" pad="100"/>
<connect gate="_" pin="IO62" pad="101"/>
<connect gate="_" pin="IO64" pad="102"/>
<connect gate="_" pin="IO65" pad="168"/>
<connect gate="_" pin="IO67" pad="169"/>
<connect gate="_" pin="IO69" pad="170"/>
<connect gate="_" pin="IO70" pad="171"/>
<connect gate="_" pin="IO72" pad="172"/>
<connect gate="_" pin="IO73" pad="173"/>
<connect gate="_" pin="IO75" pad="175"/>
<connect gate="_" pin="IO77-TDI" pad="176"/>
<connect gate="_" pin="IO78" pad="177"/>
<connect gate="_" pin="IO8" pad="161"/>
<connect gate="_" pin="IO80" pad="178"/>
<connect gate="_" pin="IO81" pad="130"/>
<connect gate="_" pin="IO83" pad="131"/>
<connect gate="_" pin="IO85" pad="132"/>
<connect gate="_" pin="IO86" pad="133"/>
<connect gate="_" pin="IO88" pad="135"/>
<connect gate="_" pin="IO89" pad="136"/>
<connect gate="_" pin="IO9" pad="162"/>
<connect gate="_" pin="IO91" pad="137"/>
<connect gate="_" pin="IO93" pad="138"/>
<connect gate="_" pin="IO94" pad="139"/>
<connect gate="_" pin="IO96" pad="140"/>
<connect gate="_" pin="IO97" pad="119"/>
<connect gate="_" pin="IO99" pad="120"/>
<connect gate="_" pin="OE1" pad="183"/>
<connect gate="_" pin="OE2-GCLK2" pad="181"/>
<connect gate="_" pin="TCK-IO173" pad="30"/>
<connect gate="_" pin="TDO-IO141" pad="189"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7256AEQC208-10N"/>
<attribute name="OC_FARNELL" value="1549440"/>
<attribute name="OC_NEWARK" value="51R9842"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7256-P192" prefix="IC">
<description>&lt;b&gt;EPM7256E&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7256R208"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCIO"/>
<gate name="V6" symbol="VCCIO"/>
<gate name="V7" symbol="VCCIO"/>
<gate name="V8" symbol="VCCIO"/>
<gate name="V9" symbol="VCCIO"/>
<gate name="V10" symbol="VCCIO"/>
<gate name="V11" symbol="VCCIO"/>
<gate name="V12" symbol="VCCIO"/>
<gate name="V13" symbol="VCCIO"/>
<gate name="V14" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="PGA192">
<connects>
<connect gate="G1" pin="GND" pad="C7"/>
<connect gate="G10" pin="GND" pad="P8"/>
<connect gate="G11" pin="GND" pad="P10"/>
<connect gate="G12" pin="GND" pad="P15"/>
<connect gate="G13" pin="GND" pad="R4"/>
<connect gate="G14" pin="GND" pad="R11"/>
<connect gate="G2" pin="GND" pad="C13"/>
<connect gate="G3" pin="GND" pad="D4"/>
<connect gate="G4" pin="GND" pad="D8"/>
<connect gate="G5" pin="GND" pad="D10"/>
<connect gate="G6" pin="GND" pad="G14"/>
<connect gate="G7" pin="GND" pad="H4"/>
<connect gate="G8" pin="GND" pad="K14"/>
<connect gate="G9" pin="GND" pad="L4"/>
<connect gate="V1" pin="VCC" pad="D7"/>
<connect gate="V10" pin="VCCIO" pad="K4"/>
<connect gate="V11" pin="VCCIO" pad="L14"/>
<connect gate="V12" pin="VCCIO" pad="P3"/>
<connect gate="V13" pin="VCCIO" pad="R5"/>
<connect gate="V14" pin="VCCIO" pad="R14"/>
<connect gate="V2" pin="VCC" pad="D11"/>
<connect gate="V3" pin="VCC" pad="P7"/>
<connect gate="V4" pin="VCC" pad="P11"/>
<connect gate="V5" pin="VCCIO" pad="C5"/>
<connect gate="V6" pin="VCCIO" pad="C11"/>
<connect gate="V7" pin="VCCIO" pad="D14"/>
<connect gate="V8" pin="VCCIO" pad="G4"/>
<connect gate="V9" pin="VCCIO" pad="H14"/>
<connect gate="_" pin="GCLK1" pad="P9"/>
<connect gate="_" pin="GCLR/" pad="R9"/>
<connect gate="_" pin="IO1" pad="U17"/>
<connect gate="_" pin="IO101" pad="F15"/>
<connect gate="_" pin="IO102" pad="G16"/>
<connect gate="_" pin="IO104" pad="G15"/>
<connect gate="_" pin="IO105" pad="G17"/>
<connect gate="_" pin="IO107" pad="H17"/>
<connect gate="_" pin="IO109-TMS" pad="H15"/>
<connect gate="_" pin="IO11" pad="T15"/>
<connect gate="_" pin="IO110" pad="J17"/>
<connect gate="_" pin="IO112" pad="H16"/>
<connect gate="_" pin="IO113" pad="C9"/>
<connect gate="_" pin="IO115" pad="D9"/>
<connect gate="_" pin="IO117" pad="C10"/>
<connect gate="_" pin="IO118" pad="A10"/>
<connect gate="_" pin="IO120" pad="A11"/>
<connect gate="_" pin="IO121" pad="B10"/>
<connect gate="_" pin="IO123" pad="A12"/>
<connect gate="_" pin="IO125" pad="B11"/>
<connect gate="_" pin="IO126" pad="A13"/>
<connect gate="_" pin="IO128" pad="C12"/>
<connect gate="_" pin="IO129" pad="U6"/>
<connect gate="_" pin="IO13" pad="U14"/>
<connect gate="_" pin="IO131" pad="T5"/>
<connect gate="_" pin="IO133" pad="U7"/>
<connect gate="_" pin="IO134" pad="T6"/>
<connect gate="_" pin="IO136" pad="T7"/>
<connect gate="_" pin="IO137" pad="R6"/>
<connect gate="_" pin="IO139" pad="R7"/>
<connect gate="_" pin="IO14" pad="U13"/>
<connect gate="_" pin="IO142" pad="R8"/>
<connect gate="_" pin="IO144" pad="T8"/>
<connect gate="_" pin="IO145" pad="J2"/>
<connect gate="_" pin="IO147" pad="J3"/>
<connect gate="_" pin="IO149" pad="K1"/>
<connect gate="_" pin="IO150" pad="J4"/>
<connect gate="_" pin="IO152" pad="K2"/>
<connect gate="_" pin="IO153" pad="K3"/>
<connect gate="_" pin="IO155" pad="L1"/>
<connect gate="_" pin="IO157" pad="L2"/>
<connect gate="_" pin="IO158" pad="M1"/>
<connect gate="_" pin="IO16" pad="T14"/>
<connect gate="_" pin="IO160" pad="L3"/>
<connect gate="_" pin="IO161" pad="F3"/>
<connect gate="_" pin="IO163" pad="F1"/>
<connect gate="_" pin="IO165" pad="E2"/>
<connect gate="_" pin="IO166" pad="G2"/>
<connect gate="_" pin="IO168" pad="G3"/>
<connect gate="_" pin="IO169" pad="G1"/>
<connect gate="_" pin="IO17" pad="N17"/>
<connect gate="_" pin="IO171" pad="H1"/>
<connect gate="_" pin="IO174" pad="J1"/>
<connect gate="_" pin="IO176" pad="H2"/>
<connect gate="_" pin="IO177" pad="B9"/>
<connect gate="_" pin="IO179" pad="C8"/>
<connect gate="_" pin="IO181" pad="A9"/>
<connect gate="_" pin="IO182" pad="A8"/>
<connect gate="_" pin="IO184" pad="A7"/>
<connect gate="_" pin="IO185" pad="B8"/>
<connect gate="_" pin="IO187" pad="A6"/>
<connect gate="_" pin="IO189" pad="B7"/>
<connect gate="_" pin="IO19" pad="M16"/>
<connect gate="_" pin="IO190" pad="A5"/>
<connect gate="_" pin="IO192" pad="C6"/>
<connect gate="_" pin="IO193" pad="U1"/>
<connect gate="_" pin="IO195" pad="R2"/>
<connect gate="_" pin="IO197" pad="R3"/>
<connect gate="_" pin="IO198" pad="U2"/>
<connect gate="_" pin="IO200" pad="P4"/>
<connect gate="_" pin="IO201" pad="U3"/>
<connect gate="_" pin="IO203" pad="T3"/>
<connect gate="_" pin="IO205" pad="U4"/>
<connect gate="_" pin="IO206" pad="U5"/>
<connect gate="_" pin="IO208" pad="T4"/>
<connect gate="_" pin="IO209" pad="N1"/>
<connect gate="_" pin="IO21" pad="M15"/>
<connect gate="_" pin="IO211" pad="M2"/>
<connect gate="_" pin="IO213" pad="M3"/>
<connect gate="_" pin="IO214" pad="P1"/>
<connect gate="_" pin="IO216" pad="N2"/>
<connect gate="_" pin="IO217" pad="R1"/>
<connect gate="_" pin="IO219" pad="P2"/>
<connect gate="_" pin="IO22" pad="P17"/>
<connect gate="_" pin="IO221" pad="T1"/>
<connect gate="_" pin="IO222" pad="N3"/>
<connect gate="_" pin="IO224" pad="T2"/>
<connect gate="_" pin="IO225" pad="B1"/>
<connect gate="_" pin="IO227" pad="C3"/>
<connect gate="_" pin="IO229" pad="C1"/>
<connect gate="_" pin="IO230" pad="D3"/>
<connect gate="_" pin="IO232" pad="D1"/>
<connect gate="_" pin="IO233" pad="C2"/>
<connect gate="_" pin="IO235" pad="E1"/>
<connect gate="_" pin="IO237" pad="E3"/>
<connect gate="_" pin="IO238" pad="D2"/>
<connect gate="_" pin="IO24" pad="N16"/>
<connect gate="_" pin="IO240" pad="F2"/>
<connect gate="_" pin="IO241" pad="A4"/>
<connect gate="_" pin="IO243" pad="B6"/>
<connect gate="_" pin="IO245" pad="B5"/>
<connect gate="_" pin="IO246" pad="A3"/>
<connect gate="_" pin="IO248" pad="B4"/>
<connect gate="_" pin="IO249" pad="A2"/>
<connect gate="_" pin="IO25" pad="R17"/>
<connect gate="_" pin="IO251" pad="C4"/>
<connect gate="_" pin="IO253" pad="B2"/>
<connect gate="_" pin="IO254" pad="B3"/>
<connect gate="_" pin="IO256" pad="A1"/>
<connect gate="_" pin="IO27" pad="P16"/>
<connect gate="_" pin="IO29" pad="T17"/>
<connect gate="_" pin="IO3" pad="R16"/>
<connect gate="_" pin="IO30" pad="N15"/>
<connect gate="_" pin="IO32" pad="T16"/>
<connect gate="_" pin="IO33" pad="B17"/>
<connect gate="_" pin="IO35" pad="C15"/>
<connect gate="_" pin="IO37" pad="C17"/>
<connect gate="_" pin="IO38" pad="C16"/>
<connect gate="_" pin="IO40" pad="D17"/>
<connect gate="_" pin="IO41" pad="D15"/>
<connect gate="_" pin="IO43" pad="E17"/>
<connect gate="_" pin="IO45" pad="D16"/>
<connect gate="_" pin="IO46" pad="E15"/>
<connect gate="_" pin="IO48" pad="F16"/>
<connect gate="_" pin="IO49" pad="A14"/>
<connect gate="_" pin="IO5" pad="P14"/>
<connect gate="_" pin="IO51" pad="B12"/>
<connect gate="_" pin="IO53" pad="B13"/>
<connect gate="_" pin="IO54" pad="A15"/>
<connect gate="_" pin="IO56" pad="B14"/>
<connect gate="_" pin="IO57" pad="A16"/>
<connect gate="_" pin="IO59" pad="C14"/>
<connect gate="_" pin="IO6" pad="U16"/>
<connect gate="_" pin="IO61" pad="B16"/>
<connect gate="_" pin="IO62" pad="B15"/>
<connect gate="_" pin="IO64" pad="A17"/>
<connect gate="_" pin="IO65" pad="U12"/>
<connect gate="_" pin="IO67" pad="R13"/>
<connect gate="_" pin="IO69" pad="U11"/>
<connect gate="_" pin="IO70" pad="T13"/>
<connect gate="_" pin="IO72" pad="T11"/>
<connect gate="_" pin="IO73" pad="T12"/>
<connect gate="_" pin="IO75" pad="R12"/>
<connect gate="_" pin="IO77-TDI" pad="U10"/>
<connect gate="_" pin="IO78" pad="R10"/>
<connect gate="_" pin="IO8" pad="R15"/>
<connect gate="_" pin="IO80" pad="T10"/>
<connect gate="_" pin="IO81" pad="J16"/>
<connect gate="_" pin="IO83" pad="J15"/>
<connect gate="_" pin="IO85" pad="K17"/>
<connect gate="_" pin="IO86" pad="J14"/>
<connect gate="_" pin="IO88" pad="K16"/>
<connect gate="_" pin="IO89" pad="K15"/>
<connect gate="_" pin="IO9" pad="U15"/>
<connect gate="_" pin="IO91" pad="L17"/>
<connect gate="_" pin="IO93" pad="L16"/>
<connect gate="_" pin="IO94" pad="M17"/>
<connect gate="_" pin="IO96" pad="L15"/>
<connect gate="_" pin="IO97" pad="E16"/>
<connect gate="_" pin="IO99" pad="F17"/>
<connect gate="_" pin="OE1" pad="T9"/>
<connect gate="_" pin="OE2-GCLK2" pad="U9"/>
<connect gate="_" pin="TCK-IO173" pad="H3"/>
<connect gate="_" pin="TDO-IO141" pad="U8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7256-P160" prefix="IC">
<description>&lt;b&gt;EPM7256E&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCIO"/>
<gate name="V6" symbol="VCCIO"/>
<gate name="V7" symbol="VCCIO"/>
<gate name="V8" symbol="VCCIO"/>
<gate name="V9" symbol="VCCIO"/>
<gate name="V10" symbol="VCCIO"/>
<gate name="V11" symbol="VCCIO"/>
<gate name="V12" symbol="VCCIO"/>
<gate name="V13" symbol="VCCIO"/>
<gate name="V14" symbol="VCCIO"/>
<gate name="_" symbol="7256P160"/>
</gates>
<devices>
<device name="" package="PQFP160">
<connects>
<connect gate="G1" pin="GND" pad="3"/>
<connect gate="G10" pin="GND" pad="111"/>
<connect gate="G11" pin="GND" pad="126"/>
<connect gate="G12" pin="GND" pad="138"/>
<connect gate="G13" pin="GND" pad="143"/>
<connect gate="G14" pin="GND" pad="148"/>
<connect gate="G2" pin="GND" pad="18"/>
<connect gate="G3" pin="GND" pad="32"/>
<connect gate="G4" pin="GND" pad="47"/>
<connect gate="G5" pin="GND" pad="57"/>
<connect gate="G6" pin="GND" pad="64"/>
<connect gate="G7" pin="GND" pad="66"/>
<connect gate="G8" pin="GND" pad="81"/>
<connect gate="G9" pin="GND" pad="96"/>
<connect gate="V1" pin="VCC" pad="56"/>
<connect gate="V10" pin="VCCIO" pad="89"/>
<connect gate="V11" pin="VCCIO" pad="103"/>
<connect gate="V12" pin="VCCIO" pad="118"/>
<connect gate="V13" pin="VCCIO" pad="133"/>
<connect gate="V14" pin="VCCIO" pad="155"/>
<connect gate="V2" pin="VCC" pad="65"/>
<connect gate="V3" pin="VCC" pad="137"/>
<connect gate="V4" pin="VCC" pad="144"/>
<connect gate="V5" pin="VCCIO" pad="10"/>
<connect gate="V6" pin="VCCIO" pad="25"/>
<connect gate="V7" pin="VCCIO" pad="40"/>
<connect gate="V8" pin="VCCIO" pad="55"/>
<connect gate="V9" pin="VCCIO" pad="74"/>
<connect gate="_" pin="GCLK1" pad="139"/>
<connect gate="_" pin="GCLR/" pad="141"/>
<connect gate="_" pin="IO1" pad="2"/>
<connect gate="_" pin="IO101" pad="28"/>
<connect gate="_" pin="IO104" pad="27"/>
<connect gate="_" pin="IO105" pad="26"/>
<connect gate="_" pin="IO107" pad="24"/>
<connect gate="_" pin="IO109-TMS" pad="23"/>
<connect gate="_" pin="IO11" pad="157"/>
<connect gate="_" pin="IO112" pad="22"/>
<connect gate="_" pin="IO113" pad="60"/>
<connect gate="_" pin="IO115" pad="59"/>
<connect gate="_" pin="IO117" pad="58"/>
<connect gate="_" pin="IO120" pad="54"/>
<connect gate="_" pin="IO121" pad="53"/>
<connect gate="_" pin="IO123" pad="52"/>
<connect gate="_" pin="IO125" pad="51"/>
<connect gate="_" pin="IO128" pad="50"/>
<connect gate="_" pin="IO129" pad="128"/>
<connect gate="_" pin="IO13" pad="156"/>
<connect gate="_" pin="IO131" pad="129"/>
<connect gate="_" pin="IO133" pad="130"/>
<connect gate="_" pin="IO136" pad="131"/>
<connect gate="_" pin="IO137" pad="132"/>
<connect gate="_" pin="IO139" pad="134"/>
<connect gate="_" pin="IO144" pad="136"/>
<connect gate="_" pin="IO145" pad="100"/>
<connect gate="_" pin="IO147" pad="101"/>
<connect gate="_" pin="IO149" pad="102"/>
<connect gate="_" pin="IO152" pad="104"/>
<connect gate="_" pin="IO153" pad="105"/>
<connect gate="_" pin="IO155" pad="106"/>
<connect gate="_" pin="IO157" pad="107"/>
<connect gate="_" pin="IO16" pad="154"/>
<connect gate="_" pin="IO160" pad="108"/>
<connect gate="_" pin="IO161" pad="91"/>
<connect gate="_" pin="IO163" pad="92"/>
<connect gate="_" pin="IO165" pad="93"/>
<connect gate="_" pin="IO168" pad="94"/>
<connect gate="_" pin="IO169" pad="95"/>
<connect gate="_" pin="IO17" pad="12"/>
<connect gate="_" pin="IO171" pad="97"/>
<connect gate="_" pin="IO176" pad="99"/>
<connect gate="_" pin="IO177" pad="61"/>
<connect gate="_" pin="IO179" pad="62"/>
<connect gate="_" pin="IO181" pad="63"/>
<connect gate="_" pin="IO184" pad="67"/>
<connect gate="_" pin="IO185" pad="68"/>
<connect gate="_" pin="IO187" pad="69"/>
<connect gate="_" pin="IO189" pad="70"/>
<connect gate="_" pin="IO19" pad="11"/>
<connect gate="_" pin="IO192" pad="71"/>
<connect gate="_" pin="IO193" pad="119"/>
<connect gate="_" pin="IO195" pad="120"/>
<connect gate="_" pin="IO197" pad="121"/>
<connect gate="_" pin="IO200" pad="122"/>
<connect gate="_" pin="IO201" pad="123"/>
<connect gate="_" pin="IO203" pad="124"/>
<connect gate="_" pin="IO205" pad="125"/>
<connect gate="_" pin="IO208" pad="127"/>
<connect gate="_" pin="IO209" pad="109"/>
<connect gate="_" pin="IO21" pad="9"/>
<connect gate="_" pin="IO211" pad="110"/>
<connect gate="_" pin="IO213" pad="112"/>
<connect gate="_" pin="IO216" pad="113"/>
<connect gate="_" pin="IO217" pad="114"/>
<connect gate="_" pin="IO219" pad="115"/>
<connect gate="_" pin="IO221" pad="116"/>
<connect gate="_" pin="IO224" pad="117"/>
<connect gate="_" pin="IO225" pad="82"/>
<connect gate="_" pin="IO227" pad="83"/>
<connect gate="_" pin="IO229" pad="84"/>
<connect gate="_" pin="IO232" pad="85"/>
<connect gate="_" pin="IO233" pad="86"/>
<connect gate="_" pin="IO235" pad="87"/>
<connect gate="_" pin="IO237" pad="88"/>
<connect gate="_" pin="IO24" pad="8"/>
<connect gate="_" pin="IO240" pad="90"/>
<connect gate="_" pin="IO241" pad="72"/>
<connect gate="_" pin="IO243" pad="73"/>
<connect gate="_" pin="IO245" pad="75"/>
<connect gate="_" pin="IO248" pad="76"/>
<connect gate="_" pin="IO249" pad="77"/>
<connect gate="_" pin="IO25" pad="7"/>
<connect gate="_" pin="IO251" pad="78"/>
<connect gate="_" pin="IO253" pad="79"/>
<connect gate="_" pin="IO256" pad="80"/>
<connect gate="_" pin="IO27" pad="6"/>
<connect gate="_" pin="IO29" pad="5"/>
<connect gate="_" pin="IO3" pad="1"/>
<connect gate="_" pin="IO32" pad="4"/>
<connect gate="_" pin="IO33" pad="39"/>
<connect gate="_" pin="IO35" pad="38"/>
<connect gate="_" pin="IO37" pad="37"/>
<connect gate="_" pin="IO40" pad="36"/>
<connect gate="_" pin="IO41" pad="35"/>
<connect gate="_" pin="IO43" pad="34"/>
<connect gate="_" pin="IO45" pad="33"/>
<connect gate="_" pin="IO48" pad="31"/>
<connect gate="_" pin="IO49" pad="49"/>
<connect gate="_" pin="IO5" pad="160"/>
<connect gate="_" pin="IO51" pad="48"/>
<connect gate="_" pin="IO53" pad="46"/>
<connect gate="_" pin="IO56" pad="45"/>
<connect gate="_" pin="IO57" pad="44"/>
<connect gate="_" pin="IO59" pad="43"/>
<connect gate="_" pin="IO61" pad="42"/>
<connect gate="_" pin="IO64" pad="41"/>
<connect gate="_" pin="IO65" pad="153"/>
<connect gate="_" pin="IO67" pad="152"/>
<connect gate="_" pin="IO69" pad="151"/>
<connect gate="_" pin="IO72" pad="150"/>
<connect gate="_" pin="IO73" pad="149"/>
<connect gate="_" pin="IO75" pad="147"/>
<connect gate="_" pin="IO77-TDI" pad="146"/>
<connect gate="_" pin="IO8" pad="159"/>
<connect gate="_" pin="IO80" pad="145"/>
<connect gate="_" pin="IO81" pad="21"/>
<connect gate="_" pin="IO83" pad="20"/>
<connect gate="_" pin="IO85" pad="19"/>
<connect gate="_" pin="IO88" pad="17"/>
<connect gate="_" pin="IO89" pad="16"/>
<connect gate="_" pin="IO9" pad="158"/>
<connect gate="_" pin="IO91" pad="15"/>
<connect gate="_" pin="IO93" pad="14"/>
<connect gate="_" pin="IO96" pad="13"/>
<connect gate="_" pin="IO97" pad="30"/>
<connect gate="_" pin="IO99" pad="29"/>
<connect gate="_" pin="OE1" pad="140"/>
<connect gate="_" pin="OE2-GCLK2" pad="142"/>
<connect gate="_" pin="TCK-IO173" pad="98"/>
<connect gate="_" pin="TDO-IO141" pad="135"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7256EQC160-12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9894"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7160-84" prefix="IC">
<description>&lt;b&gt;EPM7160E&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7160-J84"/>
<gate name="P" symbol="PWR8-2-6"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
</gates>
<devices>
<device name="" package="PLCC84">
<connects>
<connect gate="NC1" pin="NC" pad="6"/>
<connect gate="NC2" pin="NC" pad="39"/>
<connect gate="NC3" pin="NC" pad="46"/>
<connect gate="NC4" pin="NC" pad="79"/>
<connect gate="P" pin="GND" pad="7"/>
<connect gate="P" pin="GND@1" pad="19"/>
<connect gate="P" pin="GND@2" pad="32"/>
<connect gate="P" pin="GND@3" pad="42"/>
<connect gate="P" pin="GND@4" pad="47"/>
<connect gate="P" pin="GND@5" pad="59"/>
<connect gate="P" pin="GND@6" pad="72"/>
<connect gate="P" pin="GND@7" pad="82"/>
<connect gate="P" pin="VCC" pad="3"/>
<connect gate="P" pin="VCC@1" pad="43"/>
<connect gate="P" pin="VCCIO" pad="13"/>
<connect gate="P" pin="VCCIO@1" pad="26"/>
<connect gate="P" pin="VCCIO@2" pad="38"/>
<connect gate="P" pin="VCCIO@3" pad="53"/>
<connect gate="P" pin="VCCIO@4" pad="66"/>
<connect gate="P" pin="VCCIO@5" pad="78"/>
<connect gate="_" pin="GCLK1" pad="83"/>
<connect gate="_" pin="GCLR/" pad="1"/>
<connect gate="_" pin="IO1" pad="11"/>
<connect gate="_" pin="IO102" pad="54"/>
<connect gate="_" pin="IO104" pad="55"/>
<connect gate="_" pin="IO107" pad="56"/>
<connect gate="_" pin="IO11" pad="5"/>
<connect gate="_" pin="IO110" pad="57"/>
<connect gate="_" pin="IO112" pad="58"/>
<connect gate="_" pin="IO115" pad="60"/>
<connect gate="_" pin="IO118" pad="61"/>
<connect gate="_" pin="IO120" pad="62"/>
<connect gate="_" pin="IO123" pad="65"/>
<connect gate="_" pin="IO126" pad="64"/>
<connect gate="_" pin="IO128" pad="63"/>
<connect gate="_" pin="IO129" pad="67"/>
<connect gate="_" pin="IO131" pad="68"/>
<connect gate="_" pin="IO136" pad="69"/>
<connect gate="_" pin="IO137" pad="70"/>
<connect gate="_" pin="IO139" pad="71"/>
<connect gate="_" pin="IO144" pad="73"/>
<connect gate="_" pin="IO145" pad="74"/>
<connect gate="_" pin="IO147" pad="75"/>
<connect gate="_" pin="IO152" pad="76"/>
<connect gate="_" pin="IO153" pad="77"/>
<connect gate="_" pin="IO155" pad="80"/>
<connect gate="_" pin="IO16" pad="4"/>
<connect gate="_" pin="IO160" pad="81"/>
<connect gate="_" pin="IO17" pad="18"/>
<connect gate="_" pin="IO19" pad="17"/>
<connect gate="_" pin="IO24" pad="16"/>
<connect gate="_" pin="IO25" pad="15"/>
<connect gate="_" pin="IO27" pad="14"/>
<connect gate="_" pin="IO3" pad="10"/>
<connect gate="_" pin="IO32" pad="12"/>
<connect gate="_" pin="IO35" pad="25"/>
<connect gate="_" pin="IO38" pad="24"/>
<connect gate="_" pin="IO40" pad="23"/>
<connect gate="_" pin="IO43" pad="20"/>
<connect gate="_" pin="IO46" pad="21"/>
<connect gate="_" pin="IO48" pad="22"/>
<connect gate="_" pin="IO51" pad="33"/>
<connect gate="_" pin="IO54" pad="31"/>
<connect gate="_" pin="IO56" pad="30"/>
<connect gate="_" pin="IO59" pad="29"/>
<connect gate="_" pin="IO62" pad="28"/>
<connect gate="_" pin="IO64" pad="27"/>
<connect gate="_" pin="IO67" pad="41"/>
<connect gate="_" pin="IO70" pad="40"/>
<connect gate="_" pin="IO72" pad="37"/>
<connect gate="_" pin="IO75" pad="36"/>
<connect gate="_" pin="IO78" pad="35"/>
<connect gate="_" pin="IO8" pad="9"/>
<connect gate="_" pin="IO80" pad="34"/>
<connect gate="_" pin="IO83" pad="44"/>
<connect gate="_" pin="IO86" pad="45"/>
<connect gate="_" pin="IO88" pad="48"/>
<connect gate="_" pin="IO9" pad="8"/>
<connect gate="_" pin="IO91" pad="49"/>
<connect gate="_" pin="IO94" pad="50"/>
<connect gate="_" pin="IO96" pad="51"/>
<connect gate="_" pin="IO99" pad="52"/>
<connect gate="_" pin="OE1" pad="84"/>
<connect gate="_" pin="OE2-GCLK2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7160SLC84-10N"/>
<attribute name="OC_FARNELL" value="1549460"/>
<attribute name="OC_NEWARK" value="51R0533"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7160-?100" prefix="IC">
<description>&lt;b&gt;EPM7160E&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7160P100"/>
<gate name="P" symbol="PWR8-2-6"/>
</gates>
<devices>
<device name="P" package="PQFP100">
<connects>
<connect gate="P" pin="GND" pad="13"/>
<connect gate="P" pin="GND@1" pad="28"/>
<connect gate="P" pin="GND@2" pad="40"/>
<connect gate="P" pin="GND@3" pad="45"/>
<connect gate="P" pin="GND@4" pad="61"/>
<connect gate="P" pin="GND@5" pad="76"/>
<connect gate="P" pin="GND@6" pad="88"/>
<connect gate="P" pin="GND@7" pad="97"/>
<connect gate="P" pin="VCC" pad="41"/>
<connect gate="P" pin="VCC@1" pad="93"/>
<connect gate="P" pin="VCCIO" pad="5"/>
<connect gate="P" pin="VCCIO@1" pad="20"/>
<connect gate="P" pin="VCCIO@2" pad="36"/>
<connect gate="P" pin="VCCIO@3" pad="53"/>
<connect gate="P" pin="VCCIO@4" pad="68"/>
<connect gate="P" pin="VCCIO@5" pad="84"/>
<connect gate="_" pin="GCLK1" pad="89"/>
<connect gate="_" pin="GCLR/" pad="91"/>
<connect gate="_" pin="IO1" pad="2"/>
<connect gate="_" pin="IO101" pad="52"/>
<connect gate="_" pin="IO102" pad="54"/>
<connect gate="_" pin="IO104" pad="55"/>
<connect gate="_" pin="IO107" pad="56"/>
<connect gate="_" pin="IO109" pad="57"/>
<connect gate="_" pin="IO11" pad="96"/>
<connect gate="_" pin="IO110" pad="58"/>
<connect gate="_" pin="IO112" pad="59"/>
<connect gate="_" pin="IO113" pad="60"/>
<connect gate="_" pin="IO115" pad="62"/>
<connect gate="_" pin="IO118" pad="63"/>
<connect gate="_" pin="IO120" pad="64"/>
<connect gate="_" pin="IO121" pad="69"/>
<connect gate="_" pin="IO123" pad="67"/>
<connect gate="_" pin="IO126" pad="66"/>
<connect gate="_" pin="IO128" pad="65"/>
<connect gate="_" pin="IO129" pad="70"/>
<connect gate="_" pin="IO131" pad="71"/>
<connect gate="_" pin="IO134" pad="72"/>
<connect gate="_" pin="IO136" pad="73"/>
<connect gate="_" pin="IO137" pad="74"/>
<connect gate="_" pin="IO139" pad="75"/>
<connect gate="_" pin="IO14" pad="95"/>
<connect gate="_" pin="IO142" pad="77"/>
<connect gate="_" pin="IO144" pad="78"/>
<connect gate="_" pin="IO145" pad="79"/>
<connect gate="_" pin="IO147" pad="80"/>
<connect gate="_" pin="IO150" pad="81"/>
<connect gate="_" pin="IO152" pad="82"/>
<connect gate="_" pin="IO153" pad="83"/>
<connect gate="_" pin="IO155" pad="85"/>
<connect gate="_" pin="IO158" pad="86"/>
<connect gate="_" pin="IO16" pad="94"/>
<connect gate="_" pin="IO160" pad="87"/>
<connect gate="_" pin="IO17" pad="11"/>
<connect gate="_" pin="IO19" pad="10"/>
<connect gate="_" pin="IO22" pad="9"/>
<connect gate="_" pin="IO24" pad="8"/>
<connect gate="_" pin="IO25" pad="7"/>
<connect gate="_" pin="IO27" pad="6"/>
<connect gate="_" pin="IO3" pad="1"/>
<connect gate="_" pin="IO30" pad="4"/>
<connect gate="_" pin="IO32" pad="3"/>
<connect gate="_" pin="IO33" pad="21"/>
<connect gate="_" pin="IO35" pad="19"/>
<connect gate="_" pin="IO38" pad="18"/>
<connect gate="_" pin="IO40" pad="17"/>
<connect gate="_" pin="IO41" pad="12"/>
<connect gate="_" pin="IO43" pad="14"/>
<connect gate="_" pin="IO46" pad="15"/>
<connect gate="_" pin="IO48" pad="16"/>
<connect gate="_" pin="IO51" pad="30"/>
<connect gate="_" pin="IO53" pad="29"/>
<connect gate="_" pin="IO54" pad="27"/>
<connect gate="_" pin="IO56" pad="26"/>
<connect gate="_" pin="IO59" pad="25"/>
<connect gate="_" pin="IO6" pad="100"/>
<connect gate="_" pin="IO61" pad="24"/>
<connect gate="_" pin="IO62" pad="23"/>
<connect gate="_" pin="IO64" pad="22"/>
<connect gate="_" pin="IO67" pad="39"/>
<connect gate="_" pin="IO69" pad="38"/>
<connect gate="_" pin="IO70" pad="37"/>
<connect gate="_" pin="IO72" pad="35"/>
<connect gate="_" pin="IO75" pad="34"/>
<connect gate="_" pin="IO77" pad="33"/>
<connect gate="_" pin="IO78" pad="32"/>
<connect gate="_" pin="IO8" pad="99"/>
<connect gate="_" pin="IO80" pad="31"/>
<connect gate="_" pin="IO83" pad="42"/>
<connect gate="_" pin="IO85" pad="43"/>
<connect gate="_" pin="IO86" pad="44"/>
<connect gate="_" pin="IO88" pad="46"/>
<connect gate="_" pin="IO9" pad="98"/>
<connect gate="_" pin="IO91" pad="47"/>
<connect gate="_" pin="IO93" pad="48"/>
<connect gate="_" pin="IO94" pad="49"/>
<connect gate="_" pin="IO96" pad="50"/>
<connect gate="_" pin="IO99" pad="51"/>
<connect gate="_" pin="OE1" pad="90"/>
<connect gate="_" pin="OE2-GCLK2" pad="92"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7160SQC160-10N"/>
<attribute name="OC_FARNELL" value="1549437"/>
<attribute name="OC_NEWARK" value="51R9800"/>
</technology>
</technologies>
</device>
<device name="T" package="TQFP100">
<connects>
<connect gate="P" pin="GND" pad="38"/>
<connect gate="P" pin="GND@1" pad="86"/>
<connect gate="P" pin="GND@2" pad="11"/>
<connect gate="P" pin="GND@3" pad="26"/>
<connect gate="P" pin="GND@4" pad="43"/>
<connect gate="P" pin="GND@5" pad="59"/>
<connect gate="P" pin="GND@6" pad="74"/>
<connect gate="P" pin="GND@7" pad="95"/>
<connect gate="P" pin="VCC" pad="39"/>
<connect gate="P" pin="VCC@1" pad="91"/>
<connect gate="P" pin="VCCIO" pad="3"/>
<connect gate="P" pin="VCCIO@1" pad="18"/>
<connect gate="P" pin="VCCIO@2" pad="34"/>
<connect gate="P" pin="VCCIO@3" pad="51"/>
<connect gate="P" pin="VCCIO@4" pad="66"/>
<connect gate="P" pin="VCCIO@5" pad="82"/>
<connect gate="_" pin="GCLK1" pad="87"/>
<connect gate="_" pin="GCLR/" pad="89"/>
<connect gate="_" pin="IO1" pad="100"/>
<connect gate="_" pin="IO101" pad="50"/>
<connect gate="_" pin="IO102" pad="52"/>
<connect gate="_" pin="IO104" pad="53"/>
<connect gate="_" pin="IO107" pad="54"/>
<connect gate="_" pin="IO109" pad="55"/>
<connect gate="_" pin="IO11" pad="94"/>
<connect gate="_" pin="IO110" pad="56"/>
<connect gate="_" pin="IO112" pad="57"/>
<connect gate="_" pin="IO113" pad="58"/>
<connect gate="_" pin="IO115" pad="60"/>
<connect gate="_" pin="IO118" pad="61"/>
<connect gate="_" pin="IO120" pad="62"/>
<connect gate="_" pin="IO121" pad="67"/>
<connect gate="_" pin="IO123" pad="65"/>
<connect gate="_" pin="IO126" pad="64"/>
<connect gate="_" pin="IO128" pad="63"/>
<connect gate="_" pin="IO129" pad="68"/>
<connect gate="_" pin="IO131" pad="69"/>
<connect gate="_" pin="IO134" pad="70"/>
<connect gate="_" pin="IO136" pad="71"/>
<connect gate="_" pin="IO137" pad="72"/>
<connect gate="_" pin="IO139" pad="73"/>
<connect gate="_" pin="IO14" pad="93"/>
<connect gate="_" pin="IO142" pad="75"/>
<connect gate="_" pin="IO144" pad="76"/>
<connect gate="_" pin="IO145" pad="77"/>
<connect gate="_" pin="IO147" pad="78"/>
<connect gate="_" pin="IO150" pad="79"/>
<connect gate="_" pin="IO152" pad="80"/>
<connect gate="_" pin="IO153" pad="81"/>
<connect gate="_" pin="IO155" pad="83"/>
<connect gate="_" pin="IO158" pad="84"/>
<connect gate="_" pin="IO16" pad="92"/>
<connect gate="_" pin="IO160" pad="85"/>
<connect gate="_" pin="IO17" pad="9"/>
<connect gate="_" pin="IO19" pad="8"/>
<connect gate="_" pin="IO22" pad="7"/>
<connect gate="_" pin="IO24" pad="6"/>
<connect gate="_" pin="IO25" pad="5"/>
<connect gate="_" pin="IO27" pad="4"/>
<connect gate="_" pin="IO3" pad="99"/>
<connect gate="_" pin="IO30" pad="2"/>
<connect gate="_" pin="IO32" pad="1"/>
<connect gate="_" pin="IO33" pad="19"/>
<connect gate="_" pin="IO35" pad="17"/>
<connect gate="_" pin="IO38" pad="16"/>
<connect gate="_" pin="IO40" pad="15"/>
<connect gate="_" pin="IO41" pad="10"/>
<connect gate="_" pin="IO43" pad="12"/>
<connect gate="_" pin="IO46" pad="13"/>
<connect gate="_" pin="IO48" pad="14"/>
<connect gate="_" pin="IO51" pad="28"/>
<connect gate="_" pin="IO53" pad="27"/>
<connect gate="_" pin="IO54" pad="25"/>
<connect gate="_" pin="IO56" pad="24"/>
<connect gate="_" pin="IO59" pad="23"/>
<connect gate="_" pin="IO6" pad="98"/>
<connect gate="_" pin="IO61" pad="22"/>
<connect gate="_" pin="IO62" pad="21"/>
<connect gate="_" pin="IO64" pad="20"/>
<connect gate="_" pin="IO67" pad="37"/>
<connect gate="_" pin="IO69" pad="36"/>
<connect gate="_" pin="IO70" pad="35"/>
<connect gate="_" pin="IO72" pad="33"/>
<connect gate="_" pin="IO75" pad="32"/>
<connect gate="_" pin="IO77" pad="31"/>
<connect gate="_" pin="IO78" pad="30"/>
<connect gate="_" pin="IO8" pad="97"/>
<connect gate="_" pin="IO80" pad="29"/>
<connect gate="_" pin="IO83" pad="40"/>
<connect gate="_" pin="IO85" pad="41"/>
<connect gate="_" pin="IO86" pad="42"/>
<connect gate="_" pin="IO88" pad="44"/>
<connect gate="_" pin="IO9" pad="96"/>
<connect gate="_" pin="IO91" pad="45"/>
<connect gate="_" pin="IO93" pad="46"/>
<connect gate="_" pin="IO94" pad="47"/>
<connect gate="_" pin="IO96" pad="48"/>
<connect gate="_" pin="IO99" pad="49"/>
<connect gate="_" pin="OE1" pad="88"/>
<connect gate="_" pin="OE2-GCLK2" pad="90"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7160STC100-10N"/>
<attribute name="OC_FARNELL" value="1549429"/>
<attribute name="OC_NEWARK" value="51R9804"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7160-P160" prefix="IC">
<description>&lt;b&gt;EPM7160S&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="P" symbol="PWR8-2-6"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC40" symbol="NC"/>
<gate name="_" symbol="7160P160"/>
</gates>
<devices>
<device name="" package="PQFP160">
<connects>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="37"/>
<connect gate="NC11" pin="NC" pad="38"/>
<connect gate="NC12" pin="NC" pad="39"/>
<connect gate="NC13" pin="NC" pad="40"/>
<connect gate="NC14" pin="NC" pad="45"/>
<connect gate="NC15" pin="NC" pad="46"/>
<connect gate="NC16" pin="NC" pad="47"/>
<connect gate="NC17" pin="NC" pad="74"/>
<connect gate="NC18" pin="NC" pad="75"/>
<connect gate="NC19" pin="NC" pad="76"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC20" pin="NC" pad="81"/>
<connect gate="NC21" pin="NC" pad="82"/>
<connect gate="NC22" pin="NC" pad="83"/>
<connect gate="NC23" pin="NC" pad="84"/>
<connect gate="NC24" pin="NC" pad="85"/>
<connect gate="NC25" pin="NC" pad="86"/>
<connect gate="NC26" pin="NC" pad="87"/>
<connect gate="NC27" pin="NC" pad="115"/>
<connect gate="NC28" pin="NC" pad="116"/>
<connect gate="NC29" pin="NC" pad="117"/>
<connect gate="NC3" pin="NC" pad="3"/>
<connect gate="NC30" pin="NC" pad="118"/>
<connect gate="NC31" pin="NC" pad="119"/>
<connect gate="NC32" pin="NC" pad="120"/>
<connect gate="NC33" pin="NC" pad="124"/>
<connect gate="NC34" pin="NC" pad="125"/>
<connect gate="NC35" pin="NC" pad="126"/>
<connect gate="NC36" pin="NC" pad="127"/>
<connect gate="NC37" pin="NC" pad="154"/>
<connect gate="NC38" pin="NC" pad="155"/>
<connect gate="NC39" pin="NC" pad="156"/>
<connect gate="NC4" pin="NC" pad="4"/>
<connect gate="NC40" pin="NC" pad="157"/>
<connect gate="NC5" pin="NC" pad="5"/>
<connect gate="NC6" pin="NC" pad="6"/>
<connect gate="NC7" pin="NC" pad="34"/>
<connect gate="NC8" pin="NC" pad="35"/>
<connect gate="NC9" pin="NC" pad="36"/>
<connect gate="P" pin="GND" pad="17"/>
<connect gate="P" pin="GND@1" pad="42"/>
<connect gate="P" pin="GND@2" pad="60"/>
<connect gate="P" pin="GND@3" pad="66"/>
<connect gate="P" pin="GND@4" pad="95"/>
<connect gate="P" pin="GND@5" pad="113"/>
<connect gate="P" pin="GND@6" pad="138"/>
<connect gate="P" pin="GND@7" pad="148"/>
<connect gate="P" pin="VCC" pad="61"/>
<connect gate="P" pin="VCC@1" pad="143"/>
<connect gate="P" pin="VCCIO" pad="8"/>
<connect gate="P" pin="VCCIO@1" pad="26"/>
<connect gate="P" pin="VCCIO@2" pad="55"/>
<connect gate="P" pin="VCCIO@3" pad="79"/>
<connect gate="P" pin="VCCIO@4" pad="104"/>
<connect gate="P" pin="VCCIO@5" pad="133"/>
<connect gate="_" pin="GCLK1" pad="139"/>
<connect gate="_" pin="GCLR/" pad="141"/>
<connect gate="_" pin="IO1" pad="158"/>
<connect gate="_" pin="IO101" pad="78"/>
<connect gate="_" pin="IO102" pad="80"/>
<connect gate="_" pin="IO104" pad="88"/>
<connect gate="_" pin="IO105" pad="89"/>
<connect gate="_" pin="IO107" pad="90"/>
<connect gate="_" pin="IO109-TMS" pad="91"/>
<connect gate="_" pin="IO11" pad="147"/>
<connect gate="_" pin="IO110" pad="92"/>
<connect gate="_" pin="IO112" pad="93"/>
<connect gate="_" pin="IO113" pad="94"/>
<connect gate="_" pin="IO115" pad="96"/>
<connect gate="_" pin="IO117" pad="97"/>
<connect gate="_" pin="IO118" pad="98"/>
<connect gate="_" pin="IO120" pad="99"/>
<connect gate="_" pin="IO121" pad="105"/>
<connect gate="_" pin="IO123" pad="103"/>
<connect gate="_" pin="IO125" pad="102"/>
<connect gate="_" pin="IO126" pad="101"/>
<connect gate="_" pin="IO128" pad="100"/>
<connect gate="_" pin="IO129" pad="106"/>
<connect gate="_" pin="IO13" pad="146"/>
<connect gate="_" pin="IO131" pad="107"/>
<connect gate="_" pin="IO133" pad="108"/>
<connect gate="_" pin="IO134" pad="109"/>
<connect gate="_" pin="IO136" pad="110"/>
<connect gate="_" pin="IO137" pad="111"/>
<connect gate="_" pin="IO139" pad="112"/>
<connect gate="_" pin="IO14" pad="145"/>
<connect gate="_" pin="IO142" pad="121"/>
<connect gate="_" pin="IO144" pad="122"/>
<connect gate="_" pin="IO145" pad="123"/>
<connect gate="_" pin="IO147" pad="128"/>
<connect gate="_" pin="IO149" pad="129"/>
<connect gate="_" pin="IO150" pad="130"/>
<connect gate="_" pin="IO152" pad="131"/>
<connect gate="_" pin="IO153" pad="132"/>
<connect gate="_" pin="IO155" pad="134"/>
<connect gate="_" pin="IO157" pad="135"/>
<connect gate="_" pin="IO158" pad="136"/>
<connect gate="_" pin="IO16" pad="144"/>
<connect gate="_" pin="IO160" pad="137"/>
<connect gate="_" pin="IO17" pad="15"/>
<connect gate="_" pin="IO19" pad="14"/>
<connect gate="_" pin="IO21" pad="13"/>
<connect gate="_" pin="IO22" pad="12"/>
<connect gate="_" pin="IO24" pad="11"/>
<connect gate="_" pin="IO25" pad="10"/>
<connect gate="_" pin="IO27" pad="9"/>
<connect gate="_" pin="IO29" pad="7"/>
<connect gate="_" pin="IO3" pad="153"/>
<connect gate="_" pin="IO30" pad="160"/>
<connect gate="_" pin="IO32" pad="159"/>
<connect gate="_" pin="IO33" pad="27"/>
<connect gate="_" pin="IO35" pad="25"/>
<connect gate="_" pin="IO37" pad="24"/>
<connect gate="_" pin="IO38" pad="23"/>
<connect gate="_" pin="IO40" pad="22"/>
<connect gate="_" pin="IO41" pad="16"/>
<connect gate="_" pin="IO43" pad="18"/>
<connect gate="_" pin="IO45" pad="19"/>
<connect gate="_" pin="IO46" pad="20"/>
<connect gate="_" pin="IO48" pad="21"/>
<connect gate="_" pin="IO49" pad="48"/>
<connect gate="_" pin="IO5" pad="152"/>
<connect gate="_" pin="IO51" pad="44"/>
<connect gate="_" pin="IO53" pad="43"/>
<connect gate="_" pin="IO54" pad="41"/>
<connect gate="_" pin="IO56" pad="33"/>
<connect gate="_" pin="IO57" pad="32"/>
<connect gate="_" pin="IO59" pad="31"/>
<connect gate="_" pin="IO6" pad="151"/>
<connect gate="_" pin="IO61" pad="30"/>
<connect gate="_" pin="IO62" pad="29"/>
<connect gate="_" pin="IO64" pad="28"/>
<connect gate="_" pin="IO65" pad="59"/>
<connect gate="_" pin="IO67" pad="58"/>
<connect gate="_" pin="IO69" pad="57"/>
<connect gate="_" pin="IO70" pad="56"/>
<connect gate="_" pin="IO72" pad="54"/>
<connect gate="_" pin="IO73" pad="53"/>
<connect gate="_" pin="IO75" pad="52"/>
<connect gate="_" pin="IO77-TDI" pad="51"/>
<connect gate="_" pin="IO78" pad="50"/>
<connect gate="_" pin="IO8" pad="150"/>
<connect gate="_" pin="IO80" pad="49"/>
<connect gate="_" pin="IO81" pad="62"/>
<connect gate="_" pin="IO83" pad="63"/>
<connect gate="_" pin="IO85" pad="64"/>
<connect gate="_" pin="IO86" pad="65"/>
<connect gate="_" pin="IO88" pad="67"/>
<connect gate="_" pin="IO89" pad="68"/>
<connect gate="_" pin="IO9" pad="149"/>
<connect gate="_" pin="IO91" pad="69"/>
<connect gate="_" pin="IO93" pad="70"/>
<connect gate="_" pin="IO94" pad="71"/>
<connect gate="_" pin="IO96" pad="72"/>
<connect gate="_" pin="IO97" pad="73"/>
<connect gate="_" pin="IO99" pad="77"/>
<connect gate="_" pin="OE1" pad="140"/>
<connect gate="_" pin="OE2-GCLK2" pad="142"/>
<connect gate="_" pin="TDO-IO141" pad="114"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7160SQC160-10N"/>
<attribute name="OC_FARNELL" value="1549437"/>
<attribute name="OC_NEWARK" value="51R9800"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7192-PGA160" prefix="IC">
<description>&lt;b&gt;EPM7192E&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="7192"/>
</gates>
<devices>
<device name="" package="PGA160">
<connects>
<connect gate="G1" pin="GND" pad="C4"/>
<connect gate="G10" pin="GND" pad="M7"/>
<connect gate="G11" pin="GND" pad="M9"/>
<connect gate="G12" pin="GND" pad="M13"/>
<connect gate="G13" pin="GND" pad="N4"/>
<connect gate="G14" pin="GND" pad="N11"/>
<connect gate="G2" pin="GND" pad="C6"/>
<connect gate="G3" pin="GND" pad="C11"/>
<connect gate="G4" pin="GND" pad="D7"/>
<connect gate="G5" pin="GND" pad="D9"/>
<connect gate="G6" pin="GND" pad="D13"/>
<connect gate="G7" pin="GND" pad="G4"/>
<connect gate="G8" pin="GND" pad="H12"/>
<connect gate="G9" pin="GND" pad="J4"/>
<connect gate="NC1" pin="NC" pad="A1"/>
<connect gate="NC2" pin="NC" pad="A2"/>
<connect gate="NC3" pin="NC" pad="A14"/>
<connect gate="NC4" pin="NC" pad="A15"/>
<connect gate="NC5" pin="NC" pad="R1"/>
<connect gate="NC6" pin="NC" pad="R2"/>
<connect gate="NC7" pin="NC" pad="R14"/>
<connect gate="NC8" pin="NC" pad="R15"/>
<connect gate="NC9" pin="GCLK1" pad="M8"/>
<connect gate="NC9" pin="GCLR/" pad="N8"/>
<connect gate="NC9" pin="IO1" pad="M12"/>
<connect gate="NC9" pin="IO101" pad="A7"/>
<connect gate="NC9" pin="IO102" pad="A6"/>
<connect gate="NC9" pin="IO104" pad="B7"/>
<connect gate="NC9" pin="IO105" pad="A5"/>
<connect gate="NC9" pin="IO107" pad="B6"/>
<connect gate="NC9" pin="IO109" pad="A4"/>
<connect gate="NC9" pin="IO11" pad="R11"/>
<connect gate="NC9" pin="IO110" pad="B5"/>
<connect gate="NC9" pin="IO112" pad="D4"/>
<connect gate="NC9" pin="IO113" pad="A3"/>
<connect gate="NC9" pin="IO115" pad="B4"/>
<connect gate="NC9" pin="IO117" pad="B3"/>
<connect gate="NC9" pin="IO118" pad="C3"/>
<connect gate="NC9" pin="IO120" pad="B2"/>
<connect gate="NC9" pin="IO121" pad="B1"/>
<connect gate="NC9" pin="IO123" pad="C2"/>
<connect gate="NC9" pin="IO125" pad="C1"/>
<connect gate="NC9" pin="IO126" pad="D2"/>
<connect gate="NC9" pin="IO128" pad="D1"/>
<connect gate="NC9" pin="IO129" pad="E3"/>
<connect gate="NC9" pin="IO13" pad="R10"/>
<connect gate="NC9" pin="IO131" pad="F3"/>
<connect gate="NC9" pin="IO133" pad="E2"/>
<connect gate="NC9" pin="IO134" pad="F2"/>
<connect gate="NC9" pin="IO136" pad="E1"/>
<connect gate="NC9" pin="IO137" pad="G3"/>
<connect gate="NC9" pin="IO139" pad="F1"/>
<connect gate="NC9" pin="IO14" pad="P9"/>
<connect gate="NC9" pin="IO141" pad="G1"/>
<connect gate="NC9" pin="IO142" pad="G2"/>
<connect gate="NC9" pin="IO144" pad="H1"/>
<connect gate="NC9" pin="IO145" pad="H2"/>
<connect gate="NC9" pin="IO147" pad="J1"/>
<connect gate="NC9" pin="IO149" pad="H3"/>
<connect gate="NC9" pin="IO150" pad="J3"/>
<connect gate="NC9" pin="IO152" pad="K1"/>
<connect gate="NC9" pin="IO153" pad="J2"/>
<connect gate="NC9" pin="IO155" pad="K2"/>
<connect gate="NC9" pin="IO157" pad="K3"/>
<connect gate="NC9" pin="IO158" pad="L1"/>
<connect gate="NC9" pin="IO16" pad="R9"/>
<connect gate="NC9" pin="IO160" pad="M1"/>
<connect gate="NC9" pin="IO161" pad="L2"/>
<connect gate="NC9" pin="IO163" pad="N1"/>
<connect gate="NC9" pin="IO165" pad="L3"/>
<connect gate="NC9" pin="IO166" pad="P1"/>
<connect gate="NC9" pin="IO168" pad="M2"/>
<connect gate="NC9" pin="IO169" pad="N2"/>
<connect gate="NC9" pin="IO17" pad="L14"/>
<connect gate="NC9" pin="IO171" pad="P2"/>
<connect gate="NC9" pin="IO173" pad="N3"/>
<connect gate="NC9" pin="IO174" pad="P3"/>
<connect gate="NC9" pin="IO176" pad="P4"/>
<connect gate="NC9" pin="IO177" pad="R3"/>
<connect gate="NC9" pin="IO179" pad="R4"/>
<connect gate="NC9" pin="IO181" pad="M4"/>
<connect gate="NC9" pin="IO182" pad="R5"/>
<connect gate="NC9" pin="IO184" pad="P5"/>
<connect gate="NC9" pin="IO185" pad="R6"/>
<connect gate="NC9" pin="IO187" pad="P6"/>
<connect gate="NC9" pin="IO189" pad="N6"/>
<connect gate="NC9" pin="IO19" pad="M14"/>
<connect gate="NC9" pin="IO190" pad="R7"/>
<connect gate="NC9" pin="IO192" pad="P7"/>
<connect gate="NC9" pin="IO21" pad="M15"/>
<connect gate="NC9" pin="IO22" pad="N14"/>
<connect gate="NC9" pin="IO24" pad="N15"/>
<connect gate="NC9" pin="IO25" pad="P15"/>
<connect gate="NC9" pin="IO27" pad="N13"/>
<connect gate="NC9" pin="IO29" pad="P14"/>
<connect gate="NC9" pin="IO3" pad="P11"/>
<connect gate="NC9" pin="IO30" pad="P13"/>
<connect gate="NC9" pin="IO32" pad="R13"/>
<connect gate="NC9" pin="IO33" pad="H14"/>
<connect gate="NC9" pin="IO35" pad="J13"/>
<connect gate="NC9" pin="IO37" pad="H15"/>
<connect gate="NC9" pin="IO38" pad="J15"/>
<connect gate="NC9" pin="IO40" pad="J14"/>
<connect gate="NC9" pin="IO41" pad="K15"/>
<connect gate="NC9" pin="IO43" pad="K13"/>
<connect gate="NC9" pin="IO45" pad="L15"/>
<connect gate="NC9" pin="IO46" pad="K14"/>
<connect gate="NC9" pin="IO48" pad="L13"/>
<connect gate="NC9" pin="IO49" pad="D15"/>
<connect gate="NC9" pin="IO5" pad="P12"/>
<connect gate="NC9" pin="IO51" pad="E15"/>
<connect gate="NC9" pin="IO53" pad="E14"/>
<connect gate="NC9" pin="IO54" pad="F15"/>
<connect gate="NC9" pin="IO56" pad="F13"/>
<connect gate="NC9" pin="IO57" pad="G14"/>
<connect gate="NC9" pin="IO59" pad="F14"/>
<connect gate="NC9" pin="IO6" pad="P10"/>
<connect gate="NC9" pin="IO61" pad="G13"/>
<connect gate="NC9" pin="IO62" pad="G15"/>
<connect gate="NC9" pin="IO64" pad="H13"/>
<connect gate="NC9" pin="IO65" pad="B12"/>
<connect gate="NC9" pin="IO67" pad="B13"/>
<connect gate="NC9" pin="IO69" pad="C13"/>
<connect gate="NC9" pin="IO70" pad="B14"/>
<connect gate="NC9" pin="IO72" pad="C14"/>
<connect gate="NC9" pin="IO73" pad="D12"/>
<connect gate="NC9" pin="IO75" pad="B15"/>
<connect gate="NC9" pin="IO77" pad="D14"/>
<connect gate="NC9" pin="IO78" pad="C15"/>
<connect gate="NC9" pin="IO8" pad="R12"/>
<connect gate="NC9" pin="IO80" pad="E13"/>
<connect gate="NC9" pin="IO81" pad="D8"/>
<connect gate="NC9" pin="IO83" pad="A9"/>
<connect gate="NC9" pin="IO85" pad="C8"/>
<connect gate="NC9" pin="IO86" pad="B9"/>
<connect gate="NC9" pin="IO88" pad="A10"/>
<connect gate="NC9" pin="IO89" pad="B10"/>
<connect gate="NC9" pin="IO9" pad="N10"/>
<connect gate="NC9" pin="IO91" pad="A11"/>
<connect gate="NC9" pin="IO93" pad="B11"/>
<connect gate="NC9" pin="IO94" pad="A12"/>
<connect gate="NC9" pin="IO96" pad="A13"/>
<connect gate="NC9" pin="IO97" pad="A8"/>
<connect gate="NC9" pin="IO99" pad="B8"/>
<connect gate="NC9" pin="OE1" pad="P8"/>
<connect gate="NC9" pin="OE2-GCLK2" pad="R8"/>
<connect gate="V1" pin="VCC" pad="C7"/>
<connect gate="V2" pin="VCC" pad="C9"/>
<connect gate="V3" pin="VCC" pad="N7"/>
<connect gate="V4" pin="VCC" pad="N9"/>
<connect gate="VO1" pin="VCCIO" pad="C5"/>
<connect gate="VO10" pin="VCCIO" pad="N12"/>
<connect gate="VO2" pin="VCCIO" pad="C10"/>
<connect gate="VO3" pin="VCCIO" pad="C12"/>
<connect gate="VO4" pin="VCCIO" pad="D3"/>
<connect gate="VO5" pin="VCCIO" pad="G12"/>
<connect gate="VO6" pin="VCCIO" pad="H4"/>
<connect gate="VO7" pin="VCCIO" pad="J12"/>
<connect gate="VO8" pin="VCCIO" pad="M3"/>
<connect gate="VO9" pin="VCCIO" pad="N5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7192-P160" prefix="IC">
<description>&lt;b&gt;EPM7192E&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="G" symbol="7192"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
</gates>
<devices>
<device name="" package="PQFP160">
<connects>
<connect gate="G" pin="GCLK1" pad="139"/>
<connect gate="G" pin="GCLR/" pad="141"/>
<connect gate="G" pin="IO1" pad="156"/>
<connect gate="G" pin="IO101" pad="63"/>
<connect gate="G" pin="IO102" pad="68"/>
<connect gate="G" pin="IO104" pad="69"/>
<connect gate="G" pin="IO105" pad="70"/>
<connect gate="G" pin="IO107" pad="71"/>
<connect gate="G" pin="IO109" pad="72"/>
<connect gate="G" pin="IO11" pad="149"/>
<connect gate="G" pin="IO110" pad="73"/>
<connect gate="G" pin="IO112" pad="75"/>
<connect gate="G" pin="IO113" pad="76"/>
<connect gate="G" pin="IO115" pad="77"/>
<connect gate="G" pin="IO117" pad="78"/>
<connect gate="G" pin="IO118" pad="79"/>
<connect gate="G" pin="IO120" pad="80"/>
<connect gate="G" pin="IO121" pad="83"/>
<connect gate="G" pin="IO123" pad="84"/>
<connect gate="G" pin="IO125" pad="85"/>
<connect gate="G" pin="IO126" pad="86"/>
<connect gate="G" pin="IO128" pad="87"/>
<connect gate="G" pin="IO129" pad="88"/>
<connect gate="G" pin="IO13" pad="147"/>
<connect gate="G" pin="IO131" pad="90"/>
<connect gate="G" pin="IO133" pad="91"/>
<connect gate="G" pin="IO134" pad="92"/>
<connect gate="G" pin="IO136" pad="93"/>
<connect gate="G" pin="IO137" pad="94"/>
<connect gate="G" pin="IO139" pad="95"/>
<connect gate="G" pin="IO14" pad="146"/>
<connect gate="G" pin="IO141" pad="97"/>
<connect gate="G" pin="IO142" pad="98"/>
<connect gate="G" pin="IO144" pad="99"/>
<connect gate="G" pin="IO145" pad="100"/>
<connect gate="G" pin="IO147" pad="101"/>
<connect gate="G" pin="IO149" pad="102"/>
<connect gate="G" pin="IO150" pad="104"/>
<connect gate="G" pin="IO152" pad="105"/>
<connect gate="G" pin="IO153" pad="106"/>
<connect gate="G" pin="IO155" pad="107"/>
<connect gate="G" pin="IO157" pad="108"/>
<connect gate="G" pin="IO158" pad="109"/>
<connect gate="G" pin="IO16" pad="145"/>
<connect gate="G" pin="IO160" pad="112"/>
<connect gate="G" pin="IO161" pad="113"/>
<connect gate="G" pin="IO163" pad="114"/>
<connect gate="G" pin="IO165" pad="115"/>
<connect gate="G" pin="IO166" pad="116"/>
<connect gate="G" pin="IO168" pad="117"/>
<connect gate="G" pin="IO169" pad="119"/>
<connect gate="G" pin="IO17" pad="8"/>
<connect gate="G" pin="IO171" pad="121"/>
<connect gate="G" pin="IO173" pad="122"/>
<connect gate="G" pin="IO174" pad="123"/>
<connect gate="G" pin="IO176" pad="124"/>
<connect gate="G" pin="IO177" pad="125"/>
<connect gate="G" pin="IO179" pad="127"/>
<connect gate="G" pin="IO181" pad="128"/>
<connect gate="G" pin="IO182" pad="129"/>
<connect gate="G" pin="IO184" pad="130"/>
<connect gate="G" pin="IO185" pad="131"/>
<connect gate="G" pin="IO187" pad="132"/>
<connect gate="G" pin="IO189" pad="134"/>
<connect gate="G" pin="IO19" pad="7"/>
<connect gate="G" pin="IO190" pad="135"/>
<connect gate="G" pin="IO192" pad="136"/>
<connect gate="G" pin="IO21" pad="6"/>
<connect gate="G" pin="IO22" pad="5"/>
<connect gate="G" pin="IO24" pad="4"/>
<connect gate="G" pin="IO25" pad="2"/>
<connect gate="G" pin="IO27" pad="160"/>
<connect gate="G" pin="IO29" pad="159"/>
<connect gate="G" pin="IO3" pad="154"/>
<connect gate="G" pin="IO30" pad="158"/>
<connect gate="G" pin="IO32" pad="157"/>
<connect gate="G" pin="IO33" pad="21"/>
<connect gate="G" pin="IO35" pad="20"/>
<connect gate="G" pin="IO37" pad="19"/>
<connect gate="G" pin="IO38" pad="17"/>
<connect gate="G" pin="IO40" pad="16"/>
<connect gate="G" pin="IO41" pad="15"/>
<connect gate="G" pin="IO43" pad="14"/>
<connect gate="G" pin="IO45" pad="13"/>
<connect gate="G" pin="IO46" pad="12"/>
<connect gate="G" pin="IO48" pad="9"/>
<connect gate="G" pin="IO49" pad="33"/>
<connect gate="G" pin="IO5" pad="153"/>
<connect gate="G" pin="IO51" pad="31"/>
<connect gate="G" pin="IO53" pad="30"/>
<connect gate="G" pin="IO54" pad="29"/>
<connect gate="G" pin="IO56" pad="28"/>
<connect gate="G" pin="IO57" pad="27"/>
<connect gate="G" pin="IO59" pad="26"/>
<connect gate="G" pin="IO6" pad="152"/>
<connect gate="G" pin="IO61" pad="24"/>
<connect gate="G" pin="IO62" pad="23"/>
<connect gate="G" pin="IO64" pad="22"/>
<connect gate="G" pin="IO65" pad="45"/>
<connect gate="G" pin="IO67" pad="44"/>
<connect gate="G" pin="IO69" pad="43"/>
<connect gate="G" pin="IO70" pad="42"/>
<connect gate="G" pin="IO72" pad="41"/>
<connect gate="G" pin="IO73" pad="38"/>
<connect gate="G" pin="IO75" pad="37"/>
<connect gate="G" pin="IO77" pad="36"/>
<connect gate="G" pin="IO78" pad="35"/>
<connect gate="G" pin="IO8" pad="151"/>
<connect gate="G" pin="IO80" pad="34"/>
<connect gate="G" pin="IO81" pad="60"/>
<connect gate="G" pin="IO83" pad="59"/>
<connect gate="G" pin="IO85" pad="58"/>
<connect gate="G" pin="IO86" pad="53"/>
<connect gate="G" pin="IO88" pad="52"/>
<connect gate="G" pin="IO89" pad="51"/>
<connect gate="G" pin="IO9" pad="150"/>
<connect gate="G" pin="IO91" pad="50"/>
<connect gate="G" pin="IO93" pad="49"/>
<connect gate="G" pin="IO94" pad="48"/>
<connect gate="G" pin="IO96" pad="46"/>
<connect gate="G" pin="IO97" pad="61"/>
<connect gate="G" pin="IO99" pad="62"/>
<connect gate="G" pin="OE1" pad="140"/>
<connect gate="G" pin="OE2-GCLK2" pad="142"/>
<connect gate="G1" pin="GND" pad="3"/>
<connect gate="G10" pin="GND" pad="111"/>
<connect gate="G11" pin="GND" pad="126"/>
<connect gate="G12" pin="GND" pad="138"/>
<connect gate="G13" pin="GND" pad="143"/>
<connect gate="G14" pin="GND" pad="148"/>
<connect gate="G2" pin="GND" pad="18"/>
<connect gate="G3" pin="GND" pad="32"/>
<connect gate="G4" pin="GND" pad="47"/>
<connect gate="G5" pin="GND" pad="57"/>
<connect gate="G6" pin="GND" pad="64"/>
<connect gate="G7" pin="GND" pad="66"/>
<connect gate="G8" pin="GND" pad="81"/>
<connect gate="G9" pin="GND" pad="96"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC2" pin="NC" pad="11"/>
<connect gate="NC3" pin="NC" pad="39"/>
<connect gate="NC4" pin="NC" pad="54"/>
<connect gate="NC5" pin="NC" pad="67"/>
<connect gate="NC6" pin="NC" pad="82"/>
<connect gate="NC7" pin="NC" pad="110"/>
<connect gate="NC8" pin="NC" pad="120"/>
<connect gate="V1" pin="VCC" pad="56"/>
<connect gate="V2" pin="VCC" pad="65"/>
<connect gate="V3" pin="VCC" pad="137"/>
<connect gate="V4" pin="VCC" pad="144"/>
<connect gate="VO1" pin="VCCIO" pad="10"/>
<connect gate="VO10" pin="VCCIO" pad="155"/>
<connect gate="VO2" pin="VCCIO" pad="25"/>
<connect gate="VO3" pin="VCCIO" pad="40"/>
<connect gate="VO4" pin="VCCIO" pad="55"/>
<connect gate="VO5" pin="VCCIO" pad="74"/>
<connect gate="VO6" pin="VCCIO" pad="89"/>
<connect gate="VO7" pin="VCCIO" pad="103"/>
<connect gate="VO8" pin="VCCIO" pad="118"/>
<connect gate="VO9" pin="VCCIO" pad="133"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7192SQC160-10N"/>
<attribute name="OC_FARNELL" value="1549438"/>
<attribute name="OC_NEWARK" value="51R9820"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM9560-BGA356" prefix="IC">
<description>&lt;b&gt;EPM9560&lt;/b&gt;&lt;p&gt;
MAX 9000 family</description>
<gates>
<gate name="_" symbol="9560C356"/>
<gate name="-A" symbol="A16-0"/>
<gate name="-B" symbol="B16-0"/>
<gate name="-C" symbol="C16-0"/>
<gate name="-D" symbol="D16-0"/>
<gate name="-E" symbol="E16-0"/>
<gate name="-1" symbol="IO120"/>
<gate name="-2" symbol="IO220"/>
<gate name="-3" symbol="IO320"/>
<gate name="-4" symbol="IO420"/>
<gate name="-5" symbol="IO520"/>
<gate name="-F" symbol="F16-0"/>
<gate name="-G" symbol="G16-0"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC40" symbol="NC"/>
<gate name="NC41" symbol="NC"/>
<gate name="NC42" symbol="NC"/>
<gate name="NC43" symbol="NC"/>
<gate name="NC44" symbol="NC"/>
<gate name="NC45" symbol="NC"/>
<gate name="NC46" symbol="NC"/>
<gate name="NC47" symbol="NC"/>
<gate name="NC48" symbol="NC"/>
<gate name="NC49" symbol="NC"/>
<gate name="NC50" symbol="NC"/>
<gate name="NC51" symbol="NC"/>
<gate name="NC52" symbol="NC"/>
<gate name="NC53" symbol="NC"/>
<gate name="NC54" symbol="NC"/>
<gate name="NC55" symbol="NC"/>
<gate name="NC56" symbol="NC"/>
<gate name="NC57" symbol="NC"/>
<gate name="NC58" symbol="NC"/>
<gate name="NC59" symbol="NC"/>
<gate name="NC60" symbol="NC"/>
<gate name="NC61" symbol="NC"/>
<gate name="NC62" symbol="NC"/>
<gate name="NC63" symbol="NC"/>
<gate name="NC64" symbol="NC"/>
<gate name="NC65" symbol="NC"/>
<gate name="NC66" symbol="NC"/>
</gates>
<devices>
<device name="" package="BGA356">
<connects>
<connect gate="-1" pin="IO11" pad="C6"/>
<connect gate="-1" pin="IO110" pad="E5"/>
<connect gate="-1" pin="IO111" pad="AC4"/>
<connect gate="-1" pin="IO112" pad="AC5"/>
<connect gate="-1" pin="IO113" pad="AC3"/>
<connect gate="-1" pin="IO114" pad="AD2"/>
<connect gate="-1" pin="IO115" pad="AD3"/>
<connect gate="-1" pin="IO116" pad="AD5"/>
<connect gate="-1" pin="IO117" pad="AE2"/>
<connect gate="-1" pin="IO118" pad="AE3"/>
<connect gate="-1" pin="IO119" pad="AD6"/>
<connect gate="-1" pin="IO12" pad="A3"/>
<connect gate="-1" pin="IO120" pad="AF3"/>
<connect gate="-1" pin="IO13" pad="B3"/>
<connect gate="-1" pin="IO14" pad="C5"/>
<connect gate="-1" pin="IO15" pad="B2"/>
<connect gate="-1" pin="IO16" pad="C3"/>
<connect gate="-1" pin="IO17" pad="C2"/>
<connect gate="-1" pin="IO18" pad="D5"/>
<connect gate="-1" pin="IO19" pad="C1"/>
<connect gate="-2" pin="IO21" pad="A10"/>
<connect gate="-2" pin="IO210" pad="C7"/>
<connect gate="-2" pin="IO211" pad="AD7"/>
<connect gate="-2" pin="IO212" pad="AD8"/>
<connect gate="-2" pin="IO213" pad="AF6"/>
<connect gate="-2" pin="IO214" pad="AD9"/>
<connect gate="-2" pin="IO215" pad="AE8"/>
<connect gate="-2" pin="IO216" pad="AF9"/>
<connect gate="-2" pin="IO217" pad="AD10"/>
<connect gate="-2" pin="IO218" pad="AE10"/>
<connect gate="-2" pin="IO219" pad="AF10"/>
<connect gate="-2" pin="IO22" pad="A8"/>
<connect gate="-2" pin="IO220" pad="AD11"/>
<connect gate="-2" pin="IO23" pad="C10"/>
<connect gate="-2" pin="IO24" pad="A7"/>
<connect gate="-2" pin="IO25" pad="A6"/>
<connect gate="-2" pin="IO26" pad="A5"/>
<connect gate="-2" pin="IO27" pad="C9"/>
<connect gate="-2" pin="IO28" pad="A4"/>
<connect gate="-2" pin="IO29" pad="C8"/>
<connect gate="-3" pin="IO31" pad="A16"/>
<connect gate="-3" pin="IO310" pad="C11"/>
<connect gate="-3" pin="IO311" pad="AF11"/>
<connect gate="-3" pin="IO312" pad="AD12"/>
<connect gate="-3" pin="IO313" pad="AF12"/>
<connect gate="-3" pin="IO314" pad="AF13"/>
<connect gate="-3" pin="IO315" pad="AE13"/>
<connect gate="-3" pin="IO316" pad="AD14"/>
<connect gate="-3" pin="IO317" pad="AF15"/>
<connect gate="-3" pin="IO318" pad="AD15"/>
<connect gate="-3" pin="IO319" pad="AF16"/>
<connect gate="-3" pin="IO32" pad="C15"/>
<connect gate="-3" pin="IO320" pad="AD16"/>
<connect gate="-3" pin="IO33" pad="A15"/>
<connect gate="-3" pin="IO34" pad="A14"/>
<connect gate="-3" pin="IO35" pad="C14"/>
<connect gate="-3" pin="IO36" pad="C13"/>
<connect gate="-3" pin="IO37" pad="A12"/>
<connect gate="-3" pin="IO38" pad="C12"/>
<connect gate="-3" pin="IO39" pad="A11"/>
<connect gate="-4" pin="IO41" pad="C19"/>
<connect gate="-4" pin="IO410" pad="C16"/>
<connect gate="-4" pin="IO411" pad="AF17"/>
<connect gate="-4" pin="IO412" pad="AE17"/>
<connect gate="-4" pin="IO413" pad="AD17"/>
<connect gate="-4" pin="IO414" pad="AF18"/>
<connect gate="-4" pin="IO415" pad="AF21"/>
<connect gate="-4" pin="IO416" pad="AD18"/>
<connect gate="-4" pin="IO417" pad="AF22"/>
<connect gate="-4" pin="IO418" pad="AF23"/>
<connect gate="-4" pin="IO419" pad="AD19"/>
<connect gate="-4" pin="IO42" pad="A24"/>
<connect gate="-4" pin="IO420" pad="AD20"/>
<connect gate="-4" pin="IO43" pad="A23"/>
<connect gate="-4" pin="IO44" pad="C18"/>
<connect gate="-4" pin="IO45" pad="A20"/>
<connect gate="-4" pin="IO46" pad="A19"/>
<connect gate="-4" pin="IO47" pad="C17"/>
<connect gate="-4" pin="IO48" pad="B17"/>
<connect gate="-4" pin="IO49" pad="A17"/>
<connect gate="-5" pin="IO51" pad="AC22"/>
<connect gate="-5" pin="IO510" pad="C22"/>
<connect gate="-5" pin="IO511" pad="C24"/>
<connect gate="-5" pin="IO512" pad="C21"/>
<connect gate="-5" pin="IO513" pad="C20"/>
<connect gate="-5" pin="IO514" pad="AD21"/>
<connect gate="-5" pin="IO515" pad="AF24"/>
<connect gate="-5" pin="IO516" pad="AE24"/>
<connect gate="-5" pin="IO517" pad="AD22"/>
<connect gate="-5" pin="IO518" pad="AE25"/>
<connect gate="-5" pin="IO519" pad="AD24"/>
<connect gate="-5" pin="IO52" pad="AD26"/>
<connect gate="-5" pin="IO520" pad="AD25"/>
<connect gate="-5" pin="IO53" pad="AB22"/>
<connect gate="-5" pin="IO54" pad="E24"/>
<connect gate="-5" pin="IO55" pad="D25"/>
<connect gate="-5" pin="IO56" pad="D22"/>
<connect gate="-5" pin="IO57" pad="D24"/>
<connect gate="-5" pin="IO58" pad="C26"/>
<connect gate="-5" pin="IO59" pad="C25"/>
<connect gate="-A" pin="IOA1" pad="H25"/>
<connect gate="-A" pin="IOA10" pad="F3"/>
<connect gate="-A" pin="IOA11" pad="G3"/>
<connect gate="-A" pin="IOA12" pad="F26"/>
<connect gate="-A" pin="IOA13" pad="F22"/>
<connect gate="-A" pin="IOA14" pad="E3"/>
<connect gate="-A" pin="IOA15" pad="F24"/>
<connect gate="-A" pin="IOA16" pad="E2"/>
<connect gate="-A" pin="IOA2" pad="G23"/>
<connect gate="-A" pin="IOA3" pad="G22"/>
<connect gate="-A" pin="IOA4" pad="G24"/>
<connect gate="-A" pin="IOA5" pad="G5"/>
<connect gate="-A" pin="IOA6" pad="G2"/>
<connect gate="-A" pin="IOA7" pad="H5"/>
<connect gate="-A" pin="IOA8" pad="F5"/>
<connect gate="-A" pin="IOA9" pad="F25"/>
<connect gate="-B" pin="IOB1" pad="K22"/>
<connect gate="-B" pin="IOB10" pad="J3"/>
<connect gate="-B" pin="IOB11" pad="K5"/>
<connect gate="-B" pin="IOB12" pad="K24"/>
<connect gate="-B" pin="IOB13" pad="J22"/>
<connect gate="-B" pin="IOB14" pad="J24"/>
<connect gate="-B" pin="IOB15" pad="J4"/>
<connect gate="-B" pin="IOB16" pad="K23"/>
<connect gate="-B" pin="IOB2" pad="K25"/>
<connect gate="-B" pin="IOB3" pad="H22"/>
<connect gate="-B" pin="IOB4" pad="H3"/>
<connect gate="-B" pin="IOB5" pad="J2"/>
<connect gate="-B" pin="IOB6" pad="K3"/>
<connect gate="-B" pin="IOB7" pad="L5"/>
<connect gate="-B" pin="IOB8" pad="J5"/>
<connect gate="-B" pin="IOB9" pad="H24"/>
<connect gate="-C" pin="IOC1" pad="N23"/>
<connect gate="-C" pin="IOC10" pad="L25"/>
<connect gate="-C" pin="IOC11" pad="M4"/>
<connect gate="-C" pin="IOC12" pad="L1"/>
<connect gate="-C" pin="IOC13" pad="M24"/>
<connect gate="-C" pin="IOC14" pad="L22"/>
<connect gate="-C" pin="IOC15" pad="L3"/>
<connect gate="-C" pin="IOC16" pad="M5"/>
<connect gate="-C" pin="IOC2" pad="N24"/>
<connect gate="-C" pin="IOC3" pad="M22"/>
<connect gate="-C" pin="IOC4" pad="M23"/>
<connect gate="-C" pin="IOC5" pad="M3"/>
<connect gate="-C" pin="IOC6" pad="N5"/>
<connect gate="-C" pin="IOC7" pad="M2"/>
<connect gate="-C" pin="IOC8" pad="L2"/>
<connect gate="-C" pin="IOC9" pad="L24"/>
<connect gate="-D" pin="IOD1" pad="R22"/>
<connect gate="-D" pin="IOD10" pad="N22"/>
<connect gate="-D" pin="IOD11" pad="N2"/>
<connect gate="-D" pin="IOD12" pad="P22"/>
<connect gate="-D" pin="IOD13" pad="R24"/>
<connect gate="-D" pin="IOD14" pad="P24"/>
<connect gate="-D" pin="IOD15" pad="N3"/>
<connect gate="-D" pin="IOD16" pad="P5"/>
<connect gate="-D" pin="IOD2" pad="R23"/>
<connect gate="-D" pin="IOD3" pad="R25"/>
<connect gate="-D" pin="IOD4" pad="P3"/>
<connect gate="-D" pin="IOD5" pad="P2"/>
<connect gate="-D" pin="IOD6" pad="R5"/>
<connect gate="-D" pin="IOD7" pad="R4"/>
<connect gate="-D" pin="IOD8" pad="M1"/>
<connect gate="-D" pin="IOD9" pad="P25"/>
<connect gate="-E" pin="IOE1" pad="U23"/>
<connect gate="-E" pin="IOE10" pad="R26"/>
<connect gate="-E" pin="IOE11" pad="U5"/>
<connect gate="-E" pin="IOE12" pad="T2"/>
<connect gate="-E" pin="IOE13" pad="T24"/>
<connect gate="-E" pin="IOE14" pad="T22"/>
<connect gate="-E" pin="IOE15" pad="T3"/>
<connect gate="-E" pin="IOE16" pad="R3"/>
<connect gate="-E" pin="IOE2" pad="U22"/>
<connect gate="-E" pin="IOE3" pad="U25"/>
<connect gate="-E" pin="IOE4" pad="T25"/>
<connect gate="-E" pin="IOE5" pad="U3"/>
<connect gate="-E" pin="IOE6" pad="V2"/>
<connect gate="-E" pin="IOE7" pad="W1"/>
<connect gate="-E" pin="IOE8" pad="T5"/>
<connect gate="-E" pin="IOE9" pad="T26"/>
<connect gate="-F" pin="IOF1" pad="Y24"/>
<connect gate="-F" pin="IOF10" pad="V22"/>
<connect gate="-F" pin="IOF11" pad="W3"/>
<connect gate="-F" pin="IOF12" pad="V24"/>
<connect gate="-F" pin="IOF13" pad="W2"/>
<connect gate="-F" pin="IOF14" pad="V3"/>
<connect gate="-F" pin="IOF15" pad="W24"/>
<connect gate="-F" pin="IOF16" pad="W23"/>
<connect gate="-F" pin="IOF2" pad="W22"/>
<connect gate="-F" pin="IOF3" pad="Y25"/>
<connect gate="-F" pin="IOF4" pad="W5"/>
<connect gate="-F" pin="IOF5" pad="Y2"/>
<connect gate="-F" pin="IOF6" pad="Y3"/>
<connect gate="-F" pin="IOF7" pad="Y5"/>
<connect gate="-F" pin="IOF8" pad="V5"/>
<connect gate="-F" pin="IOF9" pad="U24"/>
<connect gate="-G" pin="IOG1" pad="AB24"/>
<connect gate="-G" pin="IOG10" pad="AA3"/>
<connect gate="-G" pin="IOG11" pad="AA5"/>
<connect gate="-G" pin="IOG12" pad="Y1"/>
<connect gate="-G" pin="IOG13" pad="AB2"/>
<connect gate="-G" pin="IOG14" pad="Y22"/>
<connect gate="-G" pin="IOG15" pad="AA25"/>
<connect gate="-G" pin="IOG16" pad="AC1"/>
<connect gate="-G" pin="IOG2" pad="AB25"/>
<connect gate="-G" pin="IOG3" pad="AA22"/>
<connect gate="-G" pin="IOG4" pad="AA24"/>
<connect gate="-G" pin="IOG5" pad="AB3"/>
<connect gate="-G" pin="IOG6" pad="AB5"/>
<connect gate="-G" pin="IOG7" pad="AC2"/>
<connect gate="-G" pin="IOG8" pad="Y23"/>
<connect gate="-G" pin="IOG9" pad="AA26"/>
<connect gate="G1" pin="GND" pad="AA2"/>
<connect gate="G10" pin="GND" pad="AF20"/>
<connect gate="G11" pin="GND" pad="A9"/>
<connect gate="G12" pin="GND" pad="A22"/>
<connect gate="G13" pin="GND" pad="A25"/>
<connect gate="G14" pin="GND" pad="A26"/>
<connect gate="G15" pin="GND" pad="B25"/>
<connect gate="G16" pin="GND" pad="B26"/>
<connect gate="G17" pin="GND" pad="D2"/>
<connect gate="G18" pin="GND" pad="E1"/>
<connect gate="G19" pin="GND" pad="E26"/>
<connect gate="G2" pin="GND" pad="AB1"/>
<connect gate="G20" pin="GND" pad="F2"/>
<connect gate="G21" pin="GND" pad="G1"/>
<connect gate="G22" pin="GND" pad="G25"/>
<connect gate="G23" pin="GND" pad="G26"/>
<connect gate="G24" pin="GND" pad="H2"/>
<connect gate="G25" pin="GND" pad="J1"/>
<connect gate="G26" pin="GND" pad="J25"/>
<connect gate="G27" pin="GND" pad="J26"/>
<connect gate="G28" pin="GND" pad="K2"/>
<connect gate="G29" pin="GND" pad="L26"/>
<connect gate="G3" pin="GND" pad="AB26"/>
<connect gate="G30" pin="GND" pad="M26"/>
<connect gate="G31" pin="GND" pad="N1"/>
<connect gate="G32" pin="GND" pad="N25"/>
<connect gate="G33" pin="GND" pad="P26"/>
<connect gate="G34" pin="GND" pad="R2"/>
<connect gate="G35" pin="GND" pad="T1"/>
<connect gate="G36" pin="GND" pad="U2"/>
<connect gate="G37" pin="GND" pad="U26"/>
<connect gate="G38" pin="GND" pad="V1"/>
<connect gate="G39" pin="GND" pad="V25"/>
<connect gate="G4" pin="GND" pad="AC26"/>
<connect gate="G40" pin="GND" pad="W25"/>
<connect gate="G41" pin="GND" pad="Y26"/>
<connect gate="G5" pin="GND" pad="AE1"/>
<connect gate="G6" pin="GND" pad="AF1"/>
<connect gate="G7" pin="GND" pad="AF2"/>
<connect gate="G8" pin="GND" pad="AF4"/>
<connect gate="G9" pin="GND" pad="AF7"/>
<connect gate="NC1" pin="NC" pad="AA4"/>
<connect gate="NC10" pin="NC" pad="AE6"/>
<connect gate="NC11" pin="NC" pad="AE7"/>
<connect gate="NC12" pin="NC" pad="AE9"/>
<connect gate="NC13" pin="NC" pad="AE11"/>
<connect gate="NC14" pin="NC" pad="AE12"/>
<connect gate="NC15" pin="NC" pad="AE14"/>
<connect gate="NC16" pin="NC" pad="AE15"/>
<connect gate="NC17" pin="NC" pad="AE16"/>
<connect gate="NC18" pin="NC" pad="AE18"/>
<connect gate="NC19" pin="NC" pad="AE19"/>
<connect gate="NC2" pin="NC" pad="AA23"/>
<connect gate="NC20" pin="NC" pad="AE20"/>
<connect gate="NC21" pin="NC" pad="AE21"/>
<connect gate="NC22" pin="NC" pad="AE22"/>
<connect gate="NC23" pin="NC" pad="AE23"/>
<connect gate="NC24" pin="NC" pad="B4"/>
<connect gate="NC25" pin="NC" pad="B5"/>
<connect gate="NC26" pin="NC" pad="B6"/>
<connect gate="NC27" pin="NC" pad="B7"/>
<connect gate="NC28" pin="NC" pad="B8"/>
<connect gate="NC29" pin="NC" pad="B9"/>
<connect gate="NC3" pin="NC" pad="AB4"/>
<connect gate="NC30" pin="NC" pad="B11"/>
<connect gate="NC31" pin="NC" pad="B12"/>
<connect gate="NC32" pin="NC" pad="B13"/>
<connect gate="NC33" pin="NC" pad="B14"/>
<connect gate="NC34" pin="NC" pad="B15"/>
<connect gate="NC35" pin="NC" pad="B16"/>
<connect gate="NC36" pin="NC" pad="B18"/>
<connect gate="NC37" pin="NC" pad="B19"/>
<connect gate="NC38" pin="NC" pad="B20"/>
<connect gate="NC39" pin="NC" pad="B21"/>
<connect gate="NC4" pin="NC" pad="AB23"/>
<connect gate="NC40" pin="NC" pad="B22"/>
<connect gate="NC41" pin="NC" pad="B23"/>
<connect gate="NC42" pin="NC" pad="C4"/>
<connect gate="NC43" pin="NC" pad="C23"/>
<connect gate="NC44" pin="NC" pad="D4"/>
<connect gate="NC45" pin="NC" pad="D23"/>
<connect gate="NC46" pin="NC" pad="E4"/>
<connect gate="NC47" pin="NC" pad="E22"/>
<connect gate="NC48" pin="NC" pad="F4"/>
<connect gate="NC49" pin="NC" pad="F23"/>
<connect gate="NC5" pin="NC" pad="AC23"/>
<connect gate="NC50" pin="NC" pad="G4"/>
<connect gate="NC51" pin="NC" pad="H4"/>
<connect gate="NC52" pin="NC" pad="H23"/>
<connect gate="NC53" pin="NC" pad="J23"/>
<connect gate="NC54" pin="NC" pad="K4"/>
<connect gate="NC55" pin="NC" pad="L4"/>
<connect gate="NC56" pin="NC" pad="L23"/>
<connect gate="NC57" pin="NC" pad="N4"/>
<connect gate="NC58" pin="NC" pad="P4"/>
<connect gate="NC59" pin="NC" pad="P23"/>
<connect gate="NC6" pin="NC" pad="AD4"/>
<connect gate="NC60" pin="NC" pad="T4"/>
<connect gate="NC61" pin="NC" pad="T23"/>
<connect gate="NC62" pin="NC" pad="U4"/>
<connect gate="NC63" pin="NC" pad="V4"/>
<connect gate="NC64" pin="NC" pad="V23"/>
<connect gate="NC65" pin="NC" pad="W4"/>
<connect gate="NC66" pin="NC" pad="Y4"/>
<connect gate="NC7" pin="NC" pad="AD23"/>
<connect gate="NC8" pin="NC" pad="AE4"/>
<connect gate="NC9" pin="NC" pad="AE5"/>
<connect gate="V1" pin="VCC" pad="AE26"/>
<connect gate="V10" pin="VCC" pad="U1"/>
<connect gate="V11" pin="VCC" pad="W26"/>
<connect gate="V2" pin="VCC" pad="AF25"/>
<connect gate="V3" pin="VCC" pad="AF26"/>
<connect gate="V4" pin="VCC" pad="D26"/>
<connect gate="V5" pin="VCC" pad="F1"/>
<connect gate="V6" pin="VCC" pad="H1"/>
<connect gate="V7" pin="VCC" pad="K26"/>
<connect gate="V8" pin="VCC" pad="N26"/>
<connect gate="V9" pin="VCC" pad="P1"/>
<connect gate="VO1" pin="VCCIO" pad="AA1"/>
<connect gate="VO10" pin="VCCIO" pad="B10"/>
<connect gate="VO11" pin="VCCIO" pad="B24"/>
<connect gate="VO12" pin="VCCIO" pad="D1"/>
<connect gate="VO13" pin="VCCIO" pad="H26"/>
<connect gate="VO14" pin="VCCIO" pad="K1"/>
<connect gate="VO15" pin="VCCIO" pad="M25"/>
<connect gate="VO16" pin="VCCIO" pad="R1"/>
<connect gate="VO17" pin="VCCIO" pad="V26"/>
<connect gate="VO2" pin="VCCIO" pad="AC25"/>
<connect gate="VO3" pin="VCCIO" pad="AF5"/>
<connect gate="VO4" pin="VCCIO" pad="AF8"/>
<connect gate="VO5" pin="VCCIO" pad="AF19"/>
<connect gate="VO6" pin="VCCIO" pad="A1"/>
<connect gate="VO7" pin="VCCIO" pad="A2"/>
<connect gate="VO8" pin="VCCIO" pad="A21"/>
<connect gate="VO9" pin="VCCIO" pad="B1"/>
<connect gate="_" pin="GCLK0" pad="AD13"/>
<connect gate="_" pin="GCLK1" pad="AF14"/>
<connect gate="_" pin="GCLR/" pad="AD1"/>
<connect gate="_" pin="OE/" pad="AC24"/>
<connect gate="_" pin="TCK" pad="A18"/>
<connect gate="_" pin="TDI" pad="A13"/>
<connect gate="_" pin="TDO" pad="D3"/>
<connect gate="_" pin="TMS" pad="E23"/>
<connect gate="_" pin="VPP-1" pad="E25"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM9560ABC356-10"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9960"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM9560-RQ304" prefix="IC">
<description>&lt;b&gt;EPM9560&lt;/b&gt;&lt;p&gt;
MAX 9000 family</description>
<gates>
<gate name="_" symbol="9560C356"/>
<gate name="-A" symbol="A16-0"/>
<gate name="-B" symbol="B16-0"/>
<gate name="-C" symbol="C16-0"/>
<gate name="-D" symbol="D16-0"/>
<gate name="-E" symbol="E16-0"/>
<gate name="-F" symbol="F16-0"/>
<gate name="-G" symbol="G16-0"/>
<gate name="-1" symbol="IO120"/>
<gate name="-2" symbol="IO220"/>
<gate name="-3" symbol="IO320"/>
<gate name="-4" symbol="IO420"/>
<gate name="-5" symbol="IO520"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
</gates>
<devices>
<device name="" package="RQFP304">
<connects>
<connect gate="-1" pin="IO11" pad="133"/>
<connect gate="-1" pin="IO110" pad="143"/>
<connect gate="-1" pin="IO111" pad="238"/>
<connect gate="-1" pin="IO112" pad="239"/>
<connect gate="-1" pin="IO113" pad="240"/>
<connect gate="-1" pin="IO114" pad="241"/>
<connect gate="-1" pin="IO115" pad="242"/>
<connect gate="-1" pin="IO116" pad="244"/>
<connect gate="-1" pin="IO117" pad="245"/>
<connect gate="-1" pin="IO118" pad="246"/>
<connect gate="-1" pin="IO119" pad="247"/>
<connect gate="-1" pin="IO12" pad="134"/>
<connect gate="-1" pin="IO120" pad="248"/>
<connect gate="-1" pin="IO13" pad="135"/>
<connect gate="-1" pin="IO14" pad="136"/>
<connect gate="-1" pin="IO15" pad="137"/>
<connect gate="-1" pin="IO16" pad="139"/>
<connect gate="-1" pin="IO17" pad="140"/>
<connect gate="-1" pin="IO18" pad="141"/>
<connect gate="-1" pin="IO19" pad="142"/>
<connect gate="-2" pin="IO21" pad="122"/>
<connect gate="-2" pin="IO210" pad="132"/>
<connect gate="-2" pin="IO211" pad="249"/>
<connect gate="-2" pin="IO212" pad="250"/>
<connect gate="-2" pin="IO213" pad="251"/>
<connect gate="-2" pin="IO214" pad="252"/>
<connect gate="-2" pin="IO215" pad="253"/>
<connect gate="-2" pin="IO216" pad="255"/>
<connect gate="-2" pin="IO217" pad="256"/>
<connect gate="-2" pin="IO218" pad="257"/>
<connect gate="-2" pin="IO219" pad="258"/>
<connect gate="-2" pin="IO22" pad="123"/>
<connect gate="-2" pin="IO220" pad="259"/>
<connect gate="-2" pin="IO23" pad="124"/>
<connect gate="-2" pin="IO24" pad="125"/>
<connect gate="-2" pin="IO25" pad="126"/>
<connect gate="-2" pin="IO26" pad="128"/>
<connect gate="-2" pin="IO27" pad="129"/>
<connect gate="-2" pin="IO28" pad="130"/>
<connect gate="-2" pin="IO29" pad="131"/>
<connect gate="-3" pin="IO31" pad="109"/>
<connect gate="-3" pin="IO310" pad="120"/>
<connect gate="-3" pin="IO311" pad="261"/>
<connect gate="-3" pin="IO312" pad="262"/>
<connect gate="-3" pin="IO313" pad="263"/>
<connect gate="-3" pin="IO314" pad="264"/>
<connect gate="-3" pin="IO315" pad="265"/>
<connect gate="-3" pin="IO316" pad="268"/>
<connect gate="-3" pin="IO317" pad="269"/>
<connect gate="-3" pin="IO318" pad="270"/>
<connect gate="-3" pin="IO319" pad="271"/>
<connect gate="-3" pin="IO32" pad="110"/>
<connect gate="-3" pin="IO320" pad="272"/>
<connect gate="-3" pin="IO33" pad="111"/>
<connect gate="-3" pin="IO34" pad="112"/>
<connect gate="-3" pin="IO35" pad="113"/>
<connect gate="-3" pin="IO36" pad="116"/>
<connect gate="-3" pin="IO37" pad="117"/>
<connect gate="-3" pin="IO38" pad="118"/>
<connect gate="-3" pin="IO39" pad="119"/>
<connect gate="-4" pin="IO41" pad="97"/>
<connect gate="-4" pin="IO410" pad="107"/>
<connect gate="-4" pin="IO411" pad="274"/>
<connect gate="-4" pin="IO412" pad="275"/>
<connect gate="-4" pin="IO413" pad="276"/>
<connect gate="-4" pin="IO414" pad="277"/>
<connect gate="-4" pin="IO415" pad="278"/>
<connect gate="-4" pin="IO416" pad="280"/>
<connect gate="-4" pin="IO417" pad="281"/>
<connect gate="-4" pin="IO418" pad="282"/>
<connect gate="-4" pin="IO419" pad="283"/>
<connect gate="-4" pin="IO42" pad="98"/>
<connect gate="-4" pin="IO420" pad="284"/>
<connect gate="-4" pin="IO43" pad="99"/>
<connect gate="-4" pin="IO44" pad="100"/>
<connect gate="-4" pin="IO45" pad="101"/>
<connect gate="-4" pin="IO46" pad="103"/>
<connect gate="-4" pin="IO47" pad="104"/>
<connect gate="-4" pin="IO48" pad="105"/>
<connect gate="-4" pin="IO49" pad="106"/>
<connect gate="-5" pin="IO51" pad="293"/>
<connect gate="-5" pin="IO510" pad="93"/>
<connect gate="-5" pin="IO511" pad="94"/>
<connect gate="-5" pin="IO512" pad="95"/>
<connect gate="-5" pin="IO513" pad="96"/>
<connect gate="-5" pin="IO514" pad="285"/>
<connect gate="-5" pin="IO515" pad="286"/>
<connect gate="-5" pin="IO516" pad="287"/>
<connect gate="-5" pin="IO517" pad="288"/>
<connect gate="-5" pin="IO518" pad="289"/>
<connect gate="-5" pin="IO519" pad="291"/>
<connect gate="-5" pin="IO52" pad="294"/>
<connect gate="-5" pin="IO520" pad="292"/>
<connect gate="-5" pin="IO53" pad="295"/>
<connect gate="-5" pin="IO54" pad="86"/>
<connect gate="-5" pin="IO55" pad="87"/>
<connect gate="-5" pin="IO56" pad="88"/>
<connect gate="-5" pin="IO57" pad="89"/>
<connect gate="-5" pin="IO58" pad="90"/>
<connect gate="-5" pin="IO59" pad="92"/>
<connect gate="-A" pin="IOA1" pad="64"/>
<connect gate="-A" pin="IOA10" pad="161"/>
<connect gate="-A" pin="IOA11" pad="163"/>
<connect gate="-A" pin="IOA12" pad="71"/>
<connect gate="-A" pin="IOA13" pad="70"/>
<connect gate="-A" pin="IOA14" pad="158"/>
<connect gate="-A" pin="IOA15" pad="69"/>
<connect gate="-A" pin="IOA16" pad="160"/>
<connect gate="-A" pin="IOA2" pad="65"/>
<connect gate="-A" pin="IOA3" pad="66"/>
<connect gate="-A" pin="IOA4" pad="67"/>
<connect gate="-A" pin="IOA5" pad="162"/>
<connect gate="-A" pin="IOA6" pad="164"/>
<connect gate="-A" pin="IOA7" pad="165"/>
<connect gate="-A" pin="IOA8" pad="159"/>
<connect gate="-A" pin="IOA9" pad="68"/>
<connect gate="-B" pin="IOB1" pad="54"/>
<connect gate="-B" pin="IOB10" pad="171"/>
<connect gate="-B" pin="IOB11" pad="173"/>
<connect gate="-B" pin="IOB12" pad="56"/>
<connect gate="-B" pin="IOB13" pad="58"/>
<connect gate="-B" pin="IOB14" pad="59"/>
<connect gate="-B" pin="IOB15" pad="170"/>
<connect gate="-B" pin="IOB16" pad="55"/>
<connect gate="-B" pin="IOB2" pad="57"/>
<connect gate="-B" pin="IOB3" pad="61"/>
<connect gate="-B" pin="IOB4" pad="168"/>
<connect gate="-B" pin="IOB5" pad="172"/>
<connect gate="-B" pin="IOB6" pad="174"/>
<connect gate="-B" pin="IOB7" pad="175"/>
<connect gate="-B" pin="IOB8" pad="169"/>
<connect gate="-B" pin="IOB9" pad="60"/>
<connect gate="-C" pin="IOC1" pad="44"/>
<connect gate="-C" pin="IOC10" pad="51"/>
<connect gate="-C" pin="IOC11" pad="181"/>
<connect gate="-C" pin="IOC12" pad="183"/>
<connect gate="-C" pin="IOC13" pad="48"/>
<connect gate="-C" pin="IOC14" pad="49"/>
<connect gate="-C" pin="IOC15" pad="178"/>
<connect gate="-C" pin="IOC16" pad="180"/>
<connect gate="-C" pin="IOC2" pad="45"/>
<connect gate="-C" pin="IOC3" pad="46"/>
<connect gate="-C" pin="IOC4" pad="47"/>
<connect gate="-C" pin="IOC5" pad="182"/>
<connect gate="-C" pin="IOC6" pad="184"/>
<connect gate="-C" pin="IOC7" pad="185"/>
<connect gate="-C" pin="IOC8" pad="179"/>
<connect gate="-C" pin="IOC9" pad="50"/>
<connect gate="-D" pin="IOD1" pad="34"/>
<connect gate="-D" pin="IOD10" pad="41"/>
<connect gate="-D" pin="IOD11" pad="191"/>
<connect gate="-D" pin="IOD12" pad="38"/>
<connect gate="-D" pin="IOD13" pad="36"/>
<connect gate="-D" pin="IOD14" pad="39"/>
<connect gate="-D" pin="IOD15" pad="188"/>
<connect gate="-D" pin="IOD16" pad="190"/>
<connect gate="-D" pin="IOD2" pad="35"/>
<connect gate="-D" pin="IOD3" pad="37"/>
<connect gate="-D" pin="IOD4" pad="192"/>
<connect gate="-D" pin="IOD5" pad="193"/>
<connect gate="-D" pin="IOD6" pad="194"/>
<connect gate="-D" pin="IOD7" pad="195"/>
<connect gate="-D" pin="IOD8" pad="189"/>
<connect gate="-D" pin="IOD9" pad="40"/>
<connect gate="-E" pin="IOE1" pad="24"/>
<connect gate="-E" pin="IOE10" pad="31"/>
<connect gate="-E" pin="IOE11" pad="203"/>
<connect gate="-E" pin="IOE12" pad="201"/>
<connect gate="-E" pin="IOE13" pad="28"/>
<connect gate="-E" pin="IOE14" pad="29"/>
<connect gate="-E" pin="IOE15" pad="200"/>
<connect gate="-E" pin="IOE16" pad="198"/>
<connect gate="-E" pin="IOE2" pad="25"/>
<connect gate="-E" pin="IOE3" pad="26"/>
<connect gate="-E" pin="IOE4" pad="27"/>
<connect gate="-E" pin="IOE5" pad="202"/>
<connect gate="-E" pin="IOE6" pad="204"/>
<connect gate="-E" pin="IOE7" pad="205"/>
<connect gate="-E" pin="IOE8" pad="199"/>
<connect gate="-E" pin="IOE9" pad="30"/>
<connect gate="-F" pin="IOF1" pad="14"/>
<connect gate="-F" pin="IOF10" pad="19"/>
<connect gate="-F" pin="IOF11" pad="211"/>
<connect gate="-F" pin="IOF12" pad="20"/>
<connect gate="-F" pin="IOF13" pad="210"/>
<connect gate="-F" pin="IOF14" pad="208"/>
<connect gate="-F" pin="IOF15" pad="18"/>
<connect gate="-F" pin="IOF16" pad="16"/>
<connect gate="-F" pin="IOF2" pad="15"/>
<connect gate="-F" pin="IOF3" pad="17"/>
<connect gate="-F" pin="IOF4" pad="212"/>
<connect gate="-F" pin="IOF5" pad="213"/>
<connect gate="-F" pin="IOF6" pad="214"/>
<connect gate="-F" pin="IOF7" pad="215"/>
<connect gate="-F" pin="IOF8" pad="209"/>
<connect gate="-F" pin="IOF9" pad="21"/>
<connect gate="-G" pin="IOG1" pad="4"/>
<connect gate="-G" pin="IOG10" pad="219"/>
<connect gate="-G" pin="IOG11" pad="220"/>
<connect gate="-G" pin="IOG12" pad="218"/>
<connect gate="-G" pin="IOG13" pad="221"/>
<connect gate="-G" pin="IOG14" pad="10"/>
<connect gate="-G" pin="IOG15" pad="8"/>
<connect gate="-G" pin="IOG16" pad="223"/>
<connect gate="-G" pin="IOG2" pad="5"/>
<connect gate="-G" pin="IOG3" pad="6"/>
<connect gate="-G" pin="IOG4" pad="7"/>
<connect gate="-G" pin="IOG5" pad="222"/>
<connect gate="-G" pin="IOG6" pad="224"/>
<connect gate="-G" pin="IOG7" pad="225"/>
<connect gate="-G" pin="IOG8" pad="11"/>
<connect gate="-G" pin="IOG9" pad="9"/>
<connect gate="G1" pin="GND" pad="13"/>
<connect gate="G10" pin="GND" pad="121"/>
<connect gate="G11" pin="GND" pad="138"/>
<connect gate="G12" pin="GND" pad="155"/>
<connect gate="G13" pin="GND" pad="166"/>
<connect gate="G14" pin="GND" pad="167"/>
<connect gate="G15" pin="GND" pad="186"/>
<connect gate="G16" pin="GND" pad="187"/>
<connect gate="G17" pin="GND" pad="206"/>
<connect gate="G18" pin="GND" pad="207"/>
<connect gate="G19" pin="GND" pad="226"/>
<connect gate="G2" pin="GND" pad="22"/>
<connect gate="G20" pin="GND" pad="254"/>
<connect gate="G21" pin="GND" pad="273"/>
<connect gate="G22" pin="GND" pad="290"/>
<connect gate="G3" pin="GND" pad="33"/>
<connect gate="G4" pin="GND" pad="42"/>
<connect gate="G5" pin="GND" pad="53"/>
<connect gate="G6" pin="GND" pad="62"/>
<connect gate="G7" pin="GND" pad="73"/>
<connect gate="G8" pin="GND" pad="74"/>
<connect gate="G9" pin="GND" pad="102"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="83"/>
<connect gate="NC11" pin="NC" pad="84"/>
<connect gate="NC12" pin="NC" pad="145"/>
<connect gate="NC13" pin="NC" pad="146"/>
<connect gate="NC14" pin="NC" pad="147"/>
<connect gate="NC15" pin="NC" pad="148"/>
<connect gate="NC16" pin="NC" pad="149"/>
<connect gate="NC17" pin="NC" pad="150"/>
<connect gate="NC18" pin="NC" pad="151"/>
<connect gate="NC19" pin="NC" pad="152"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC20" pin="NC" pad="153"/>
<connect gate="NC21" pin="NC" pad="154"/>
<connect gate="NC22" pin="NC" pad="227"/>
<connect gate="NC23" pin="NC" pad="228"/>
<connect gate="NC24" pin="NC" pad="229"/>
<connect gate="NC25" pin="NC" pad="230"/>
<connect gate="NC26" pin="NC" pad="231"/>
<connect gate="NC27" pin="NC" pad="232"/>
<connect gate="NC28" pin="NC" pad="233"/>
<connect gate="NC29" pin="NC" pad="234"/>
<connect gate="NC3" pin="NC" pad="76"/>
<connect gate="NC30" pin="NC" pad="235"/>
<connect gate="NC31" pin="NC" pad="236"/>
<connect gate="NC32" pin="NC" pad="297"/>
<connect gate="NC33" pin="NC" pad="298"/>
<connect gate="NC34" pin="NC" pad="299"/>
<connect gate="NC35" pin="NC" pad="300"/>
<connect gate="NC36" pin="NC" pad="301"/>
<connect gate="NC37" pin="NC" pad="302"/>
<connect gate="NC38" pin="NC" pad="303"/>
<connect gate="NC39" pin="NC" pad="304"/>
<connect gate="NC4" pin="NC" pad="77"/>
<connect gate="NC5" pin="NC" pad="78"/>
<connect gate="NC6" pin="NC" pad="79"/>
<connect gate="NC7" pin="NC" pad="80"/>
<connect gate="NC8" pin="NC" pad="81"/>
<connect gate="NC9" pin="NC" pad="82"/>
<connect gate="V1" pin="VCC" pad="12"/>
<connect gate="V2" pin="VCC" pad="32"/>
<connect gate="V3" pin="VCC" pad="52"/>
<connect gate="V4" pin="VCC" pad="72"/>
<connect gate="V5" pin="VCC" pad="157"/>
<connect gate="V6" pin="VCC" pad="177"/>
<connect gate="V7" pin="VCC" pad="197"/>
<connect gate="V8" pin="VCC" pad="217"/>
<connect gate="VO1" pin="VCCIO" pad="3"/>
<connect gate="VO10" pin="VCCIO" pad="196"/>
<connect gate="VO11" pin="VCCIO" pad="216"/>
<connect gate="VO12" pin="VCCIO" pad="243"/>
<connect gate="VO13" pin="VCCIO" pad="260"/>
<connect gate="VO14" pin="VCCIO" pad="279"/>
<connect gate="VO2" pin="VCCIO" pad="23"/>
<connect gate="VO3" pin="VCCIO" pad="43"/>
<connect gate="VO4" pin="VCCIO" pad="63"/>
<connect gate="VO5" pin="VCCIO" pad="91"/>
<connect gate="VO6" pin="VCCIO" pad="108"/>
<connect gate="VO7" pin="VCCIO" pad="127"/>
<connect gate="VO8" pin="VCCIO" pad="156"/>
<connect gate="VO9" pin="VCCIO" pad="176"/>
<connect gate="_" pin="GCLK0" pad="266"/>
<connect gate="_" pin="GCLK1" pad="267"/>
<connect gate="_" pin="GCLR/" pad="237"/>
<connect gate="_" pin="OE/" pad="296"/>
<connect gate="_" pin="TCK" pad="114"/>
<connect gate="_" pin="TDI" pad="115"/>
<connect gate="_" pin="TDO" pad="144"/>
<connect gate="_" pin="TMS" pad="85"/>
<connect gate="_" pin="VPP-1" pad="75"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM9560-PQ208" prefix="IC">
<description>&lt;b&gt;EPM9560&lt;/b&gt;&lt;p&gt;
MAX 9000 family</description>
<gates>
<gate name="_" symbol="9560C356"/>
<gate name="-A" symbol="A7"/>
<gate name="-B" symbol="B7"/>
<gate name="-C" symbol="C7"/>
<gate name="-D" symbol="D7"/>
<gate name="-E" symbol="E7"/>
<gate name="-F" symbol="F7"/>
<gate name="-G" symbol="G7"/>
<gate name="-1" symbol="IO120"/>
<gate name="-2" symbol="IO220"/>
<gate name="-3" symbol="IO320"/>
<gate name="-4" symbol="IO420"/>
<gate name="-5" symbol="IO520"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="-1" pin="IO11" pad="97"/>
<connect gate="-1" pin="IO110" pad="107"/>
<connect gate="-1" pin="IO111" pad="154"/>
<connect gate="-1" pin="IO112" pad="155"/>
<connect gate="-1" pin="IO113" pad="156"/>
<connect gate="-1" pin="IO114" pad="157"/>
<connect gate="-1" pin="IO115" pad="158"/>
<connect gate="-1" pin="IO116" pad="160"/>
<connect gate="-1" pin="IO117" pad="161"/>
<connect gate="-1" pin="IO118" pad="162"/>
<connect gate="-1" pin="IO119" pad="163"/>
<connect gate="-1" pin="IO12" pad="98"/>
<connect gate="-1" pin="IO120" pad="164"/>
<connect gate="-1" pin="IO13" pad="99"/>
<connect gate="-1" pin="IO14" pad="100"/>
<connect gate="-1" pin="IO15" pad="101"/>
<connect gate="-1" pin="IO16" pad="103"/>
<connect gate="-1" pin="IO17" pad="104"/>
<connect gate="-1" pin="IO18" pad="105"/>
<connect gate="-1" pin="IO19" pad="106"/>
<connect gate="-2" pin="IO21" pad="86"/>
<connect gate="-2" pin="IO210" pad="96"/>
<connect gate="-2" pin="IO211" pad="165"/>
<connect gate="-2" pin="IO212" pad="166"/>
<connect gate="-2" pin="IO213" pad="167"/>
<connect gate="-2" pin="IO214" pad="168"/>
<connect gate="-2" pin="IO215" pad="169"/>
<connect gate="-2" pin="IO216" pad="171"/>
<connect gate="-2" pin="IO217" pad="172"/>
<connect gate="-2" pin="IO218" pad="173"/>
<connect gate="-2" pin="IO219" pad="174"/>
<connect gate="-2" pin="IO22" pad="87"/>
<connect gate="-2" pin="IO220" pad="175"/>
<connect gate="-2" pin="IO23" pad="88"/>
<connect gate="-2" pin="IO24" pad="89"/>
<connect gate="-2" pin="IO25" pad="90"/>
<connect gate="-2" pin="IO26" pad="92"/>
<connect gate="-2" pin="IO27" pad="93"/>
<connect gate="-2" pin="IO28" pad="94"/>
<connect gate="-2" pin="IO29" pad="95"/>
<connect gate="-3" pin="IO31" pad="73"/>
<connect gate="-3" pin="IO310" pad="84"/>
<connect gate="-3" pin="IO311" pad="177"/>
<connect gate="-3" pin="IO312" pad="178"/>
<connect gate="-3" pin="IO313" pad="179"/>
<connect gate="-3" pin="IO314" pad="180"/>
<connect gate="-3" pin="IO315" pad="181"/>
<connect gate="-3" pin="IO316" pad="184"/>
<connect gate="-3" pin="IO317" pad="185"/>
<connect gate="-3" pin="IO318" pad="186"/>
<connect gate="-3" pin="IO319" pad="187"/>
<connect gate="-3" pin="IO32" pad="74"/>
<connect gate="-3" pin="IO320" pad="188"/>
<connect gate="-3" pin="IO33" pad="75"/>
<connect gate="-3" pin="IO34" pad="76"/>
<connect gate="-3" pin="IO35" pad="77"/>
<connect gate="-3" pin="IO36" pad="80"/>
<connect gate="-3" pin="IO37" pad="81"/>
<connect gate="-3" pin="IO38" pad="82"/>
<connect gate="-3" pin="IO39" pad="83"/>
<connect gate="-4" pin="IO41" pad="61"/>
<connect gate="-4" pin="IO410" pad="71"/>
<connect gate="-4" pin="IO411" pad="190"/>
<connect gate="-4" pin="IO412" pad="191"/>
<connect gate="-4" pin="IO413" pad="192"/>
<connect gate="-4" pin="IO414" pad="193"/>
<connect gate="-4" pin="IO415" pad="194"/>
<connect gate="-4" pin="IO416" pad="196"/>
<connect gate="-4" pin="IO417" pad="197"/>
<connect gate="-4" pin="IO418" pad="198"/>
<connect gate="-4" pin="IO419" pad="199"/>
<connect gate="-4" pin="IO42" pad="62"/>
<connect gate="-4" pin="IO420" pad="200"/>
<connect gate="-4" pin="IO43" pad="63"/>
<connect gate="-4" pin="IO44" pad="64"/>
<connect gate="-4" pin="IO45" pad="65"/>
<connect gate="-4" pin="IO46" pad="67"/>
<connect gate="-4" pin="IO47" pad="68"/>
<connect gate="-4" pin="IO48" pad="69"/>
<connect gate="-4" pin="IO49" pad="70"/>
<connect gate="-5" pin="IO51" pad="1"/>
<connect gate="-5" pin="IO510" pad="57"/>
<connect gate="-5" pin="IO511" pad="58"/>
<connect gate="-5" pin="IO512" pad="59"/>
<connect gate="-5" pin="IO513" pad="60"/>
<connect gate="-5" pin="IO514" pad="201"/>
<connect gate="-5" pin="IO515" pad="202"/>
<connect gate="-5" pin="IO516" pad="203"/>
<connect gate="-5" pin="IO517" pad="204"/>
<connect gate="-5" pin="IO518" pad="205"/>
<connect gate="-5" pin="IO519" pad="207"/>
<connect gate="-5" pin="IO52" pad="2"/>
<connect gate="-5" pin="IO520" pad="208"/>
<connect gate="-5" pin="IO53" pad="3"/>
<connect gate="-5" pin="IO54" pad="50"/>
<connect gate="-5" pin="IO55" pad="51"/>
<connect gate="-5" pin="IO56" pad="52"/>
<connect gate="-5" pin="IO57" pad="53"/>
<connect gate="-5" pin="IO58" pad="54"/>
<connect gate="-5" pin="IO59" pad="56"/>
<connect gate="-A" pin="IOA1" pad="37"/>
<connect gate="-A" pin="IOA2" pad="38"/>
<connect gate="-A" pin="IOA3" pad="39"/>
<connect gate="-A" pin="IOA4" pad="40"/>
<connect gate="-A" pin="IOA5" pad="117"/>
<connect gate="-A" pin="IOA6" pad="119"/>
<connect gate="-A" pin="IOA7" pad="120"/>
<connect gate="-B" pin="IOB1" pad="32"/>
<connect gate="-B" pin="IOB2" pad="33"/>
<connect gate="-B" pin="IOB3" pad="34"/>
<connect gate="-B" pin="IOB4" pad="123"/>
<connect gate="-B" pin="IOB5" pad="124"/>
<connect gate="-B" pin="IOB6" pad="125"/>
<connect gate="-B" pin="IOB7" pad="126"/>
<connect gate="-C" pin="IOC1" pad="26"/>
<connect gate="-C" pin="IOC2" pad="27"/>
<connect gate="-C" pin="IOC3" pad="28"/>
<connect gate="-C" pin="IOC4" pad="29"/>
<connect gate="-C" pin="IOC5" pad="129"/>
<connect gate="-C" pin="IOC6" pad="130"/>
<connect gate="-C" pin="IOC7" pad="131"/>
<connect gate="-D" pin="IOD1" pad="21"/>
<connect gate="-D" pin="IOD2" pad="22"/>
<connect gate="-D" pin="IOD3" pad="23"/>
<connect gate="-D" pin="IOD4" pad="134"/>
<connect gate="-D" pin="IOD5" pad="135"/>
<connect gate="-D" pin="IOD6" pad="136"/>
<connect gate="-D" pin="IOD7" pad="137"/>
<connect gate="-E" pin="IOE1" pad="15"/>
<connect gate="-E" pin="IOE2" pad="16"/>
<connect gate="-E" pin="IOE3" pad="17"/>
<connect gate="-E" pin="IOE4" pad="18"/>
<connect gate="-E" pin="IOE5" pad="140"/>
<connect gate="-E" pin="IOE6" pad="141"/>
<connect gate="-E" pin="IOE7" pad="142"/>
<connect gate="-F" pin="IOF1" pad="11"/>
<connect gate="-F" pin="IOF2" pad="12"/>
<connect gate="-F" pin="IOF3" pad="13"/>
<connect gate="-F" pin="IOF4" pad="144"/>
<connect gate="-F" pin="IOF5" pad="145"/>
<connect gate="-F" pin="IOF6" pad="146"/>
<connect gate="-F" pin="IOF7" pad="147"/>
<connect gate="-G" pin="IOG1" pad="6"/>
<connect gate="-G" pin="IOG2" pad="7"/>
<connect gate="-G" pin="IOG3" pad="8"/>
<connect gate="-G" pin="IOG4" pad="9"/>
<connect gate="-G" pin="IOG5" pad="149"/>
<connect gate="-G" pin="IOG6" pad="150"/>
<connect gate="-G" pin="IOG7" pad="151"/>
<connect gate="G1" pin="GND" pad="14"/>
<connect gate="G10" pin="GND" pad="46"/>
<connect gate="G11" pin="GND" pad="47"/>
<connect gate="G12" pin="GND" pad="66"/>
<connect gate="G13" pin="GND" pad="85"/>
<connect gate="G14" pin="GND" pad="102"/>
<connect gate="G15" pin="GND" pad="110"/>
<connect gate="G16" pin="GND" pad="113"/>
<connect gate="G17" pin="GND" pad="114"/>
<connect gate="G18" pin="GND" pad="115"/>
<connect gate="G19" pin="GND" pad="116"/>
<connect gate="G2" pin="GND" pad="20"/>
<connect gate="G20" pin="GND" pad="118"/>
<connect gate="G21" pin="GND" pad="121"/>
<connect gate="G22" pin="GND" pad="122"/>
<connect gate="G23" pin="GND" pad="132"/>
<connect gate="G24" pin="GND" pad="133"/>
<connect gate="G25" pin="GND" pad="143"/>
<connect gate="G26" pin="GND" pad="152"/>
<connect gate="G27" pin="GND" pad="170"/>
<connect gate="G28" pin="GND" pad="189"/>
<connect gate="G29" pin="GND" pad="206"/>
<connect gate="G3" pin="GND" pad="24"/>
<connect gate="G4" pin="GND" pad="31"/>
<connect gate="G5" pin="GND" pad="35"/>
<connect gate="G6" pin="GND" pad="41"/>
<connect gate="G7" pin="GND" pad="42"/>
<connect gate="G8" pin="GND" pad="43"/>
<connect gate="G9" pin="GND" pad="44"/>
<connect gate="NC1" pin="NC" pad="109"/>
<connect gate="V1" pin="VCC" pad="10"/>
<connect gate="V2" pin="VCC" pad="19"/>
<connect gate="V3" pin="VCC" pad="30"/>
<connect gate="V4" pin="VCC" pad="45"/>
<connect gate="V5" pin="VCC" pad="112"/>
<connect gate="V6" pin="VCC" pad="128"/>
<connect gate="V7" pin="VCC" pad="139"/>
<connect gate="V8" pin="VCC" pad="148"/>
<connect gate="VO1" pin="VCCIO" pad="5"/>
<connect gate="VO10" pin="VCCIO" pad="159"/>
<connect gate="VO11" pin="VCCIO" pad="176"/>
<connect gate="VO12" pin="VCCIO" pad="195"/>
<connect gate="VO2" pin="VCCIO" pad="25"/>
<connect gate="VO3" pin="VCCIO" pad="36"/>
<connect gate="VO4" pin="VCCIO" pad="55"/>
<connect gate="VO5" pin="VCCIO" pad="72"/>
<connect gate="VO6" pin="VCCIO" pad="91"/>
<connect gate="VO7" pin="VCCIO" pad="111"/>
<connect gate="VO8" pin="VCCIO" pad="127"/>
<connect gate="VO9" pin="VCCIO" pad="138"/>
<connect gate="_" pin="GCLK0" pad="182"/>
<connect gate="_" pin="GCLK1" pad="183"/>
<connect gate="_" pin="GCLR/" pad="153"/>
<connect gate="_" pin="OE/" pad="4"/>
<connect gate="_" pin="TCK" pad="78"/>
<connect gate="_" pin="TDI" pad="79"/>
<connect gate="_" pin="TDO" pad="108"/>
<connect gate="_" pin="TMS" pad="49"/>
<connect gate="_" pin="VPP-1" pad="48"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM9560ARC208-10"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9961"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM9560-PQ240" prefix="IC">
<description>&lt;b&gt;EPM9560&lt;/b&gt;&lt;p&gt;
MAX 9000 family</description>
<gates>
<gate name="_" symbol="9560C356"/>
<gate name="-A" symbol="A16-0"/>
<gate name="-B" symbol="B16-0"/>
<gate name="-C" symbol="C16-0"/>
<gate name="-D" symbol="D16-0"/>
<gate name="-E" symbol="E16-0"/>
<gate name="-F" symbol="F16-0"/>
<gate name="-G" symbol="G16-0"/>
<gate name="-1" symbol="IO120-2"/>
<gate name="-2" symbol="IO220-2"/>
<gate name="-3" symbol="IO320-2"/>
<gate name="-4" symbol="IO420-2"/>
<gate name="-5" symbol="IO520-2"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
</gates>
<devices>
<device name="" package="PQFP240">
<connects>
<connect gate="-1" pin="IO11" pad="106"/>
<connect gate="-1" pin="IO110" pad="113"/>
<connect gate="-1" pin="IO111" pad="188"/>
<connect gate="-1" pin="IO113" pad="189"/>
<connect gate="-1" pin="IO114" pad="190"/>
<connect gate="-1" pin="IO115" pad="191"/>
<connect gate="-1" pin="IO116" pad="193"/>
<connect gate="-1" pin="IO117" pad="194"/>
<connect gate="-1" pin="IO119" pad="195"/>
<connect gate="-1" pin="IO120" pad="196"/>
<connect gate="-1" pin="IO13" pad="107"/>
<connect gate="-1" pin="IO14" pad="108"/>
<connect gate="-1" pin="IO15" pad="109"/>
<connect gate="-1" pin="IO17" pad="111"/>
<connect gate="-1" pin="IO19" pad="112"/>
<connect gate="-2" pin="IO21" pad="97"/>
<connect gate="-2" pin="IO210" pad="105"/>
<connect gate="-2" pin="IO211" pad="197"/>
<connect gate="-2" pin="IO213" pad="198"/>
<connect gate="-2" pin="IO215" pad="199"/>
<connect gate="-2" pin="IO216" pad="201"/>
<connect gate="-2" pin="IO217" pad="202"/>
<connect gate="-2" pin="IO219" pad="203"/>
<connect gate="-2" pin="IO220" pad="204"/>
<connect gate="-2" pin="IO23" pad="98"/>
<connect gate="-2" pin="IO24" pad="99"/>
<connect gate="-2" pin="IO25" pad="100"/>
<connect gate="-2" pin="IO26" pad="102"/>
<connect gate="-2" pin="IO27" pad="103"/>
<connect gate="-2" pin="IO29" pad="104"/>
<connect gate="-3" pin="IO31" pad="87"/>
<connect gate="-3" pin="IO310" pad="95"/>
<connect gate="-3" pin="IO311" pad="206"/>
<connect gate="-3" pin="IO313" pad="207"/>
<connect gate="-3" pin="IO314" pad="208"/>
<connect gate="-3" pin="IO315" pad="209"/>
<connect gate="-3" pin="IO316" pad="212"/>
<connect gate="-3" pin="IO317" pad="213"/>
<connect gate="-3" pin="IO319" pad="214"/>
<connect gate="-3" pin="IO320" pad="215"/>
<connect gate="-3" pin="IO33" pad="88"/>
<connect gate="-3" pin="IO34" pad="89"/>
<connect gate="-3" pin="IO35" pad="90"/>
<connect gate="-3" pin="IO37" pad="93"/>
<connect gate="-3" pin="IO39" pad="94"/>
<connect gate="-4" pin="IO41" pad="77"/>
<connect gate="-4" pin="IO410" pad="85"/>
<connect gate="-4" pin="IO411" pad="217"/>
<connect gate="-4" pin="IO413" pad="218"/>
<connect gate="-4" pin="IO415" pad="219"/>
<connect gate="-4" pin="IO416" pad="221"/>
<connect gate="-4" pin="IO417" pad="222"/>
<connect gate="-4" pin="IO419" pad="223"/>
<connect gate="-4" pin="IO420" pad="224"/>
<connect gate="-4" pin="IO43" pad="78"/>
<connect gate="-4" pin="IO44" pad="79"/>
<connect gate="-4" pin="IO45" pad="80"/>
<connect gate="-4" pin="IO46" pad="82"/>
<connect gate="-4" pin="IO47" pad="83"/>
<connect gate="-4" pin="IO49" pad="84"/>
<connect gate="-5" pin="IO510" pad="74"/>
<connect gate="-5" pin="IO512" pad="75"/>
<connect gate="-5" pin="IO513" pad="76"/>
<connect gate="-5" pin="IO514" pad="225"/>
<connect gate="-5" pin="IO516" pad="226"/>
<connect gate="-5" pin="IO517" pad="227"/>
<connect gate="-5" pin="IO518" pad="228"/>
<connect gate="-5" pin="IO519" pad="230"/>
<connect gate="-5" pin="IO52" pad="232"/>
<connect gate="-5" pin="IO520" pad="231"/>
<connect gate="-5" pin="IO53" pad="233"/>
<connect gate="-5" pin="IO54" pad="69"/>
<connect gate="-5" pin="IO56" pad="70"/>
<connect gate="-5" pin="IO57" pad="71"/>
<connect gate="-5" pin="IO58" pad="72"/>
<connect gate="-A" pin="IOA1" pad="56"/>
<connect gate="-A" pin="IOA10" pad="121"/>
<connect gate="-A" pin="IOA11" pad="123"/>
<connect gate="-A" pin="IOA12" pad="63"/>
<connect gate="-A" pin="IOA13" pad="62"/>
<connect gate="-A" pin="IOA14" pad="118"/>
<connect gate="-A" pin="IOA15" pad="61"/>
<connect gate="-A" pin="IOA16" pad="120"/>
<connect gate="-A" pin="IOA2" pad="57"/>
<connect gate="-A" pin="IOA3" pad="58"/>
<connect gate="-A" pin="IOA4" pad="59"/>
<connect gate="-A" pin="IOA5" pad="122"/>
<connect gate="-A" pin="IOA6" pad="124"/>
<connect gate="-A" pin="IOA7" pad="125"/>
<connect gate="-A" pin="IOA8" pad="119"/>
<connect gate="-A" pin="IOA9" pad="60"/>
<connect gate="-B" pin="IOB1" pad="46"/>
<connect gate="-B" pin="IOB10" pad="131"/>
<connect gate="-B" pin="IOB11" pad="133"/>
<connect gate="-B" pin="IOB12" pad="48"/>
<connect gate="-B" pin="IOB13" pad="50"/>
<connect gate="-B" pin="IOB14" pad="51"/>
<connect gate="-B" pin="IOB15" pad="130"/>
<connect gate="-B" pin="IOB16" pad="47"/>
<connect gate="-B" pin="IOB2" pad="49"/>
<connect gate="-B" pin="IOB3" pad="53"/>
<connect gate="-B" pin="IOB4" pad="128"/>
<connect gate="-B" pin="IOB5" pad="132"/>
<connect gate="-B" pin="IOB6" pad="134"/>
<connect gate="-B" pin="IOB7" pad="135"/>
<connect gate="-B" pin="IOB8" pad="129"/>
<connect gate="-B" pin="IOB9" pad="52"/>
<connect gate="-C" pin="IOC1" pad="36"/>
<connect gate="-C" pin="IOC10" pad="43"/>
<connect gate="-C" pin="IOC11" pad="141"/>
<connect gate="-C" pin="IOC12" pad="143"/>
<connect gate="-C" pin="IOC13" pad="40"/>
<connect gate="-C" pin="IOC14" pad="41"/>
<connect gate="-C" pin="IOC15" pad="138"/>
<connect gate="-C" pin="IOC16" pad="140"/>
<connect gate="-C" pin="IOC2" pad="37"/>
<connect gate="-C" pin="IOC3" pad="38"/>
<connect gate="-C" pin="IOC4" pad="39"/>
<connect gate="-C" pin="IOC5" pad="142"/>
<connect gate="-C" pin="IOC6" pad="144"/>
<connect gate="-C" pin="IOC7" pad="145"/>
<connect gate="-C" pin="IOC8" pad="139"/>
<connect gate="-C" pin="IOC9" pad="42"/>
<connect gate="-D" pin="IOD1" pad="26"/>
<connect gate="-D" pin="IOD10" pad="33"/>
<connect gate="-D" pin="IOD11" pad="151"/>
<connect gate="-D" pin="IOD12" pad="30"/>
<connect gate="-D" pin="IOD13" pad="28"/>
<connect gate="-D" pin="IOD14" pad="31"/>
<connect gate="-D" pin="IOD15" pad="148"/>
<connect gate="-D" pin="IOD16" pad="150"/>
<connect gate="-D" pin="IOD2" pad="27"/>
<connect gate="-D" pin="IOD3" pad="29"/>
<connect gate="-D" pin="IOD4" pad="152"/>
<connect gate="-D" pin="IOD5" pad="153"/>
<connect gate="-D" pin="IOD6" pad="154"/>
<connect gate="-D" pin="IOD7" pad="155"/>
<connect gate="-D" pin="IOD8" pad="149"/>
<connect gate="-D" pin="IOD9" pad="32"/>
<connect gate="-E" pin="IOE1" pad="16"/>
<connect gate="-E" pin="IOE10" pad="23"/>
<connect gate="-E" pin="IOE11" pad="163"/>
<connect gate="-E" pin="IOE12" pad="161"/>
<connect gate="-E" pin="IOE13" pad="20"/>
<connect gate="-E" pin="IOE14" pad="21"/>
<connect gate="-E" pin="IOE15" pad="160"/>
<connect gate="-E" pin="IOE16" pad="158"/>
<connect gate="-E" pin="IOE2" pad="17"/>
<connect gate="-E" pin="IOE3" pad="18"/>
<connect gate="-E" pin="IOE4" pad="19"/>
<connect gate="-E" pin="IOE5" pad="162"/>
<connect gate="-E" pin="IOE6" pad="164"/>
<connect gate="-E" pin="IOE7" pad="165"/>
<connect gate="-E" pin="IOE8" pad="159"/>
<connect gate="-E" pin="IOE9" pad="22"/>
<connect gate="-F" pin="IOF1" pad="6"/>
<connect gate="-F" pin="IOF10" pad="11"/>
<connect gate="-F" pin="IOF11" pad="171"/>
<connect gate="-F" pin="IOF12" pad="12"/>
<connect gate="-F" pin="IOF13" pad="170"/>
<connect gate="-F" pin="IOF14" pad="168"/>
<connect gate="-F" pin="IOF15" pad="10"/>
<connect gate="-F" pin="IOF16" pad="8"/>
<connect gate="-F" pin="IOF2" pad="7"/>
<connect gate="-F" pin="IOF3" pad="9"/>
<connect gate="-F" pin="IOF4" pad="172"/>
<connect gate="-F" pin="IOF5" pad="173"/>
<connect gate="-F" pin="IOF6" pad="174"/>
<connect gate="-F" pin="IOF7" pad="175"/>
<connect gate="-F" pin="IOF8" pad="169"/>
<connect gate="-F" pin="IOF9" pad="13"/>
<connect gate="-G" pin="IOG1" pad="236"/>
<connect gate="-G" pin="IOG10" pad="179"/>
<connect gate="-G" pin="IOG11" pad="180"/>
<connect gate="-G" pin="IOG12" pad="178"/>
<connect gate="-G" pin="IOG13" pad="181"/>
<connect gate="-G" pin="IOG14" pad="2"/>
<connect gate="-G" pin="IOG15" pad="240"/>
<connect gate="-G" pin="IOG16" pad="183"/>
<connect gate="-G" pin="IOG2" pad="237"/>
<connect gate="-G" pin="IOG3" pad="238"/>
<connect gate="-G" pin="IOG4" pad="239"/>
<connect gate="-G" pin="IOG5" pad="182"/>
<connect gate="-G" pin="IOG6" pad="184"/>
<connect gate="-G" pin="IOG7" pad="185"/>
<connect gate="-G" pin="IOG8" pad="3"/>
<connect gate="-G" pin="IOG9" pad="1"/>
<connect gate="G1" pin="GND" pad="5"/>
<connect gate="G10" pin="GND" pad="96"/>
<connect gate="G11" pin="GND" pad="110"/>
<connect gate="G12" pin="GND" pad="115"/>
<connect gate="G13" pin="GND" pad="126"/>
<connect gate="G14" pin="GND" pad="127"/>
<connect gate="G15" pin="GND" pad="146"/>
<connect gate="G16" pin="GND" pad="147"/>
<connect gate="G17" pin="GND" pad="166"/>
<connect gate="G18" pin="GND" pad="167"/>
<connect gate="G19" pin="GND" pad="186"/>
<connect gate="G2" pin="GND" pad="14"/>
<connect gate="G20" pin="GND" pad="200"/>
<connect gate="G21" pin="GND" pad="216"/>
<connect gate="G22" pin="GND" pad="229"/>
<connect gate="G3" pin="GND" pad="25"/>
<connect gate="G4" pin="GND" pad="34"/>
<connect gate="G5" pin="GND" pad="45"/>
<connect gate="G6" pin="GND" pad="54"/>
<connect gate="G7" pin="GND" pad="65"/>
<connect gate="G8" pin="GND" pad="66"/>
<connect gate="G9" pin="GND" pad="81"/>
<connect gate="V1" pin="VCC" pad="4"/>
<connect gate="V2" pin="VCC" pad="24"/>
<connect gate="V3" pin="VCC" pad="44"/>
<connect gate="V4" pin="VCC" pad="64"/>
<connect gate="V5" pin="VCC" pad="117"/>
<connect gate="V6" pin="VCC" pad="137"/>
<connect gate="V7" pin="VCC" pad="157"/>
<connect gate="V8" pin="VCC" pad="177"/>
<connect gate="VO1" pin="VCCIO" pad="15"/>
<connect gate="VO10" pin="VCCIO" pad="176"/>
<connect gate="VO11" pin="VCCIO" pad="192"/>
<connect gate="VO12" pin="VCCIO" pad="205"/>
<connect gate="VO13" pin="VCCIO" pad="220"/>
<connect gate="VO14" pin="VCCIO" pad="235"/>
<connect gate="VO2" pin="VCCIO" pad="35"/>
<connect gate="VO3" pin="VCCIO" pad="55"/>
<connect gate="VO4" pin="VCCIO" pad="73"/>
<connect gate="VO5" pin="VCCIO" pad="86"/>
<connect gate="VO6" pin="VCCIO" pad="101"/>
<connect gate="VO7" pin="VCCIO" pad="116"/>
<connect gate="VO8" pin="VCCIO" pad="136"/>
<connect gate="VO9" pin="VCCIO" pad="156"/>
<connect gate="_" pin="GCLK0" pad="210"/>
<connect gate="_" pin="GCLK1" pad="211"/>
<connect gate="_" pin="GCLR/" pad="187"/>
<connect gate="_" pin="OE/" pad="234"/>
<connect gate="_" pin="TCK" pad="91"/>
<connect gate="_" pin="TDI" pad="92"/>
<connect gate="_" pin="TDO" pad="114"/>
<connect gate="_" pin="TMS" pad="68"/>
<connect gate="_" pin="VPP-1" pad="67"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM9560ARC240-10"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9963"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM9560-P280" prefix="IC">
<description>&lt;b&gt;EPM9560&lt;/b&gt;&lt;p&gt;
MAX 9000 family</description>
<gates>
<gate name="_" symbol="9560C356"/>
<gate name="-A" symbol="A16-0"/>
<gate name="-B" symbol="B16-0"/>
<gate name="-C" symbol="C16-0"/>
<gate name="-D" symbol="D16-0"/>
<gate name="-E" symbol="E16-0"/>
<gate name="-F" symbol="F16-0"/>
<gate name="-G" symbol="G16-0"/>
<gate name="-1" symbol="IO120"/>
<gate name="-2" symbol="IO220"/>
<gate name="-3" symbol="IO320"/>
<gate name="-4" symbol="IO420"/>
<gate name="-5" symbol="IO520"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
</gates>
<devices>
<device name="" package="PGA280">
<connects>
<connect gate="-1" pin="IO11" pad="B14"/>
<connect gate="-1" pin="IO110" pad="C17"/>
<connect gate="-1" pin="IO111" pad="W19"/>
<connect gate="-1" pin="IO112" pad="U16"/>
<connect gate="-1" pin="IO113" pad="V18"/>
<connect gate="-1" pin="IO114" pad="V16"/>
<connect gate="-1" pin="IO115" pad="W18"/>
<connect gate="-1" pin="IO116" pad="W17"/>
<connect gate="-1" pin="IO117" pad="U15"/>
<connect gate="-1" pin="IO118" pad="W16"/>
<connect gate="-1" pin="IO119" pad="V15"/>
<connect gate="-1" pin="IO12" pad="B15"/>
<connect gate="-1" pin="IO120" pad="W15"/>
<connect gate="-1" pin="IO13" pad="C15"/>
<connect gate="-1" pin="IO14" pad="A15"/>
<connect gate="-1" pin="IO15" pad="B16"/>
<connect gate="-1" pin="IO16" pad="C16"/>
<connect gate="-1" pin="IO17" pad="A16"/>
<connect gate="-1" pin="IO18" pad="B17"/>
<connect gate="-1" pin="IO19" pad="A17"/>
<connect gate="-2" pin="IO21" pad="B11"/>
<connect gate="-2" pin="IO210" pad="A14"/>
<connect gate="-2" pin="IO211" pad="U14"/>
<connect gate="-2" pin="IO212" pad="W14"/>
<connect gate="-2" pin="IO213" pad="V14"/>
<connect gate="-2" pin="IO214" pad="W13"/>
<connect gate="-2" pin="IO215" pad="T12"/>
<connect gate="-2" pin="IO216" pad="U13"/>
<connect gate="-2" pin="IO217" pad="V12"/>
<connect gate="-2" pin="IO218" pad="V13"/>
<connect gate="-2" pin="IO219" pad="W12"/>
<connect gate="-2" pin="IO22" pad="C13"/>
<connect gate="-2" pin="IO220" pad="T11"/>
<connect gate="-2" pin="IO23" pad="A12"/>
<connect gate="-2" pin="IO24" pad="D12"/>
<connect gate="-2" pin="IO25" pad="B12"/>
<connect gate="-2" pin="IO26" pad="A13"/>
<connect gate="-2" pin="IO27" pad="D13"/>
<connect gate="-2" pin="IO28" pad="B13"/>
<connect gate="-2" pin="IO29" pad="C14"/>
<connect gate="-3" pin="IO31" pad="B9"/>
<connect gate="-3" pin="IO310" pad="A11"/>
<connect gate="-3" pin="IO311" pad="U12"/>
<connect gate="-3" pin="IO312" pad="V11"/>
<connect gate="-3" pin="IO313" pad="T10"/>
<connect gate="-3" pin="IO314" pad="W11"/>
<connect gate="-3" pin="IO315" pad="U11"/>
<connect gate="-3" pin="IO316" pad="W10"/>
<connect gate="-3" pin="IO317" pad="U9"/>
<connect gate="-3" pin="IO318" pad="W9"/>
<connect gate="-3" pin="IO319" pad="T9"/>
<connect gate="-3" pin="IO32" pad="A7"/>
<connect gate="-3" pin="IO320" pad="V9"/>
<connect gate="-3" pin="IO33" pad="D10"/>
<connect gate="-3" pin="IO34" pad="A8"/>
<connect gate="-3" pin="IO35" pad="C10"/>
<connect gate="-3" pin="IO36" pad="B10"/>
<connect gate="-3" pin="IO37" pad="D11"/>
<connect gate="-3" pin="IO38" pad="A10"/>
<connect gate="-3" pin="IO39" pad="C12"/>
<connect gate="-4" pin="IO41" pad="C7"/>
<connect gate="-4" pin="IO410" pad="B8"/>
<connect gate="-4" pin="IO411" pad="W8"/>
<connect gate="-4" pin="IO412" pad="V8"/>
<connect gate="-4" pin="IO413" pad="W7"/>
<connect gate="-4" pin="IO414" pad="U8"/>
<connect gate="-4" pin="IO415" pad="W6"/>
<connect gate="-4" pin="IO416" pad="V6"/>
<connect gate="-4" pin="IO417" pad="V7"/>
<connect gate="-4" pin="IO418" pad="W5"/>
<connect gate="-4" pin="IO419" pad="T8"/>
<connect gate="-4" pin="IO42" pad="B5"/>
<connect gate="-4" pin="IO420" pad="V5"/>
<connect gate="-4" pin="IO43" pad="B7"/>
<connect gate="-4" pin="IO44" pad="A4"/>
<connect gate="-4" pin="IO45" pad="C8"/>
<connect gate="-4" pin="IO46" pad="D9"/>
<connect gate="-4" pin="IO47" pad="A5"/>
<connect gate="-4" pin="IO48" pad="C9"/>
<connect gate="-4" pin="IO49" pad="A6"/>
<connect gate="-5" pin="IO51" pad="T6"/>
<connect gate="-5" pin="IO510" pad="D7"/>
<connect gate="-5" pin="IO511" pad="B4"/>
<connect gate="-5" pin="IO512" pad="D8"/>
<connect gate="-5" pin="IO513" pad="A3"/>
<connect gate="-5" pin="IO514" pad="U7"/>
<connect gate="-5" pin="IO515" pad="W4"/>
<connect gate="-5" pin="IO516" pad="T7"/>
<connect gate="-5" pin="IO517" pad="V4"/>
<connect gate="-5" pin="IO518" pad="U6"/>
<connect gate="-5" pin="IO519" pad="U5"/>
<connect gate="-5" pin="IO52" pad="V3"/>
<connect gate="-5" pin="IO520" pad="W3"/>
<connect gate="-5" pin="IO53" pad="U4"/>
<connect gate="-5" pin="IO54" pad="B2"/>
<connect gate="-5" pin="IO55" pad="C5"/>
<connect gate="-5" pin="IO56" pad="A1"/>
<connect gate="-5" pin="IO57" pad="C6"/>
<connect gate="-5" pin="IO58" pad="B3"/>
<connect gate="-5" pin="IO59" pad="A2"/>
<connect gate="-A" pin="IOA1" pad="D1"/>
<connect gate="-A" pin="IOA10" pad="B18"/>
<connect gate="-A" pin="IOA11" pad="B19"/>
<connect gate="-A" pin="IOA12" pad="C2"/>
<connect gate="-A" pin="IOA13" pad="C3"/>
<connect gate="-A" pin="IOA14" pad="C18"/>
<connect gate="-A" pin="IOA15" pad="D3"/>
<connect gate="-A" pin="IOA16" pad="D17"/>
<connect gate="-A" pin="IOA2" pad="E3"/>
<connect gate="-A" pin="IOA3" pad="C1"/>
<connect gate="-A" pin="IOA4" pad="D2"/>
<connect gate="-A" pin="IOA5" pad="D18"/>
<connect gate="-A" pin="IOA6" pad="E17"/>
<connect gate="-A" pin="IOA7" pad="C19"/>
<connect gate="-A" pin="IOA8" pad="A19"/>
<connect gate="-A" pin="IOA9" pad="B1"/>
<connect gate="-B" pin="IOB1" pad="G2"/>
<connect gate="-B" pin="IOB10" pad="E18"/>
<connect gate="-B" pin="IOB11" pad="E19"/>
<connect gate="-B" pin="IOB12" pad="F1"/>
<connect gate="-B" pin="IOB13" pad="F2"/>
<connect gate="-B" pin="IOB14" pad="F4"/>
<connect gate="-B" pin="IOB15" pad="F17"/>
<connect gate="-B" pin="IOB16" pad="G4"/>
<connect gate="-B" pin="IOB2" pad="F3"/>
<connect gate="-B" pin="IOB3" pad="E2"/>
<connect gate="-B" pin="IOB4" pad="F16"/>
<connect gate="-B" pin="IOB5" pad="G16"/>
<connect gate="-B" pin="IOB6" pad="G17"/>
<connect gate="-B" pin="IOB7" pad="F18"/>
<connect gate="-B" pin="IOB8" pad="D19"/>
<connect gate="-B" pin="IOB9" pad="E1"/>
<connect gate="-C" pin="IOC1" pad="J2"/>
<connect gate="-C" pin="IOC10" pad="G3"/>
<connect gate="-C" pin="IOC11" pad="G18"/>
<connect gate="-C" pin="IOC12" pad="G19"/>
<connect gate="-C" pin="IOC13" pad="H2"/>
<connect gate="-C" pin="IOC14" pad="H4"/>
<connect gate="-C" pin="IOC15" pad="H16"/>
<connect gate="-C" pin="IOC16" pad="H17"/>
<connect gate="-C" pin="IOC2" pad="J4"/>
<connect gate="-C" pin="IOC3" pad="H1"/>
<connect gate="-C" pin="IOC4" pad="H3"/>
<connect gate="-C" pin="IOC5" pad="J16"/>
<connect gate="-C" pin="IOC6" pad="J17"/>
<connect gate="-C" pin="IOC7" pad="H18"/>
<connect gate="-C" pin="IOC8" pad="F19"/>
<connect gate="-C" pin="IOC9" pad="G1"/>
<connect gate="-D" pin="IOD1" pad="L1"/>
<connect gate="-D" pin="IOD10" pad="J3"/>
<connect gate="-D" pin="IOD11" pad="J18"/>
<connect gate="-D" pin="IOD12" pad="K1"/>
<connect gate="-D" pin="IOD13" pad="K2"/>
<connect gate="-D" pin="IOD14" pad="K3"/>
<connect gate="-D" pin="IOD15" pad="K16"/>
<connect gate="-D" pin="IOD16" pad="K17"/>
<connect gate="-D" pin="IOD2" pad="L3"/>
<connect gate="-D" pin="IOD3" pad="K4"/>
<connect gate="-D" pin="IOD4" pad="L17"/>
<connect gate="-D" pin="IOD5" pad="J19"/>
<connect gate="-D" pin="IOD6" pad="L16"/>
<connect gate="-D" pin="IOD7" pad="K18"/>
<connect gate="-D" pin="IOD8" pad="H19"/>
<connect gate="-D" pin="IOD9" pad="J1"/>
<connect gate="-E" pin="IOE1" pad="N1"/>
<connect gate="-E" pin="IOE10" pad="L4"/>
<connect gate="-E" pin="IOE11" pad="L18"/>
<connect gate="-E" pin="IOE12" pad="L19"/>
<connect gate="-E" pin="IOE13" pad="M1"/>
<connect gate="-E" pin="IOE14" pad="M3"/>
<connect gate="-E" pin="IOE15" pad="M16"/>
<connect gate="-E" pin="IOE16" pad="M17"/>
<connect gate="-E" pin="IOE2" pad="N2"/>
<connect gate="-E" pin="IOE3" pad="M2"/>
<connect gate="-E" pin="IOE4" pad="M4"/>
<connect gate="-E" pin="IOE5" pad="N17"/>
<connect gate="-E" pin="IOE6" pad="N16"/>
<connect gate="-E" pin="IOE7" pad="M19"/>
<connect gate="-E" pin="IOE8" pad="K19"/>
<connect gate="-E" pin="IOE9" pad="L2"/>
<connect gate="-F" pin="IOF1" pad="T2"/>
<connect gate="-F" pin="IOF10" pad="N4"/>
<connect gate="-F" pin="IOF11" pad="N19"/>
<connect gate="-F" pin="IOF12" pad="P1"/>
<connect gate="-F" pin="IOF13" pad="P17"/>
<connect gate="-F" pin="IOF14" pad="P18"/>
<connect gate="-F" pin="IOF15" pad="R1"/>
<connect gate="-F" pin="IOF16" pad="T1"/>
<connect gate="-F" pin="IOF2" pad="P3"/>
<connect gate="-F" pin="IOF3" pad="P2"/>
<connect gate="-F" pin="IOF4" pad="R18"/>
<connect gate="-F" pin="IOF5" pad="N18"/>
<connect gate="-F" pin="IOF6" pad="R17"/>
<connect gate="-F" pin="IOF7" pad="P19"/>
<connect gate="-F" pin="IOF8" pad="M18"/>
<connect gate="-F" pin="IOF9" pad="N3"/>
<connect gate="-G" pin="IOG1" pad="V2"/>
<connect gate="-G" pin="IOG10" pad="R19"/>
<connect gate="-G" pin="IOG11" pad="T17"/>
<connect gate="-G" pin="IOG12" pad="T18"/>
<connect gate="-G" pin="IOG13" pad="T19"/>
<connect gate="-G" pin="IOG14" pad="U1"/>
<connect gate="-G" pin="IOG15" pad="U2"/>
<connect gate="-G" pin="IOG16" pad="U19"/>
<connect gate="-G" pin="IOG2" pad="U3"/>
<connect gate="-G" pin="IOG3" pad="V1"/>
<connect gate="-G" pin="IOG4" pad="T3"/>
<connect gate="-G" pin="IOG5" pad="U18"/>
<connect gate="-G" pin="IOG6" pad="U17"/>
<connect gate="-G" pin="IOG7" pad="V19"/>
<connect gate="-G" pin="IOG8" pad="R2"/>
<connect gate="-G" pin="IOG9" pad="R3"/>
<connect gate="G1" pin="GND" pad="D4"/>
<connect gate="G10" pin="GND" pad="F15"/>
<connect gate="G11" pin="GND" pad="G5"/>
<connect gate="G12" pin="GND" pad="G15"/>
<connect gate="G13" pin="GND" pad="H5"/>
<connect gate="G14" pin="GND" pad="H15"/>
<connect gate="G15" pin="GND" pad="J5"/>
<connect gate="G16" pin="GND" pad="J15"/>
<connect gate="G17" pin="GND" pad="K5"/>
<connect gate="G18" pin="GND" pad="K15"/>
<connect gate="G19" pin="GND" pad="L5"/>
<connect gate="G2" pin="GND" pad="D5"/>
<connect gate="G20" pin="GND" pad="L15"/>
<connect gate="G21" pin="GND" pad="M5"/>
<connect gate="G22" pin="GND" pad="M15"/>
<connect gate="G23" pin="GND" pad="N5"/>
<connect gate="G24" pin="GND" pad="N15"/>
<connect gate="G25" pin="GND" pad="P4"/>
<connect gate="G26" pin="GND" pad="P5"/>
<connect gate="G27" pin="GND" pad="P15"/>
<connect gate="G28" pin="GND" pad="P16"/>
<connect gate="G29" pin="GND" pad="R4"/>
<connect gate="G3" pin="GND" pad="D16"/>
<connect gate="G30" pin="GND" pad="R5"/>
<connect gate="G31" pin="GND" pad="R15"/>
<connect gate="G32" pin="GND" pad="R16"/>
<connect gate="G33" pin="GND" pad="T4"/>
<connect gate="G34" pin="GND" pad="T5"/>
<connect gate="G35" pin="GND" pad="T16"/>
<connect gate="G4" pin="GND" pad="E4"/>
<connect gate="G5" pin="GND" pad="E5"/>
<connect gate="G6" pin="GND" pad="E6"/>
<connect gate="G7" pin="GND" pad="E15"/>
<connect gate="G8" pin="GND" pad="E16"/>
<connect gate="G9" pin="GND" pad="F5"/>
<connect gate="NC1" pin="NC" pad="B6"/>
<connect gate="NC2" pin="NC" pad="W1"/>
<connect gate="V1" pin="VCC" pad="D15"/>
<connect gate="V10" pin="VCC" pad="R14"/>
<connect gate="V11" pin="VCC" pad="T14"/>
<connect gate="V2" pin="VCC" pad="E8"/>
<connect gate="V3" pin="VCC" pad="E10"/>
<connect gate="V4" pin="VCC" pad="E12"/>
<connect gate="V5" pin="VCC" pad="E14"/>
<connect gate="V6" pin="VCC" pad="R7"/>
<connect gate="V7" pin="VCC" pad="R9"/>
<connect gate="V8" pin="VCC" pad="R11"/>
<connect gate="V9" pin="VCC" pad="R13"/>
<connect gate="VO1" pin="VCCIO" pad="D14"/>
<connect gate="VO10" pin="VCCIO" pad="T13"/>
<connect gate="VO11" pin="VCCIO" pad="T15"/>
<connect gate="VO2" pin="VCCIO" pad="E7"/>
<connect gate="VO3" pin="VCCIO" pad="E9"/>
<connect gate="VO4" pin="VCCIO" pad="E11"/>
<connect gate="VO5" pin="VCCIO" pad="E13"/>
<connect gate="VO6" pin="VCCIO" pad="R6"/>
<connect gate="VO7" pin="VCCIO" pad="R8"/>
<connect gate="VO8" pin="VCCIO" pad="R10"/>
<connect gate="VO9" pin="VCCIO" pad="R12"/>
<connect gate="_" pin="GCLK0" pad="V10"/>
<connect gate="_" pin="GCLK1" pad="U10"/>
<connect gate="_" pin="GCLR/" pad="V17"/>
<connect gate="_" pin="OE/" pad="W2"/>
<connect gate="_" pin="TCK" pad="A9"/>
<connect gate="_" pin="TDI" pad="C11"/>
<connect gate="_" pin="TDO" pad="A18"/>
<connect gate="_" pin="TMS" pad="D6"/>
<connect gate="_" pin="VPP-1" pad="C4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30B-FBGA256" prefix="IC">
<description>&lt;b&gt;EPF10K30B&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_1" symbol="K10-CTRL"/>
<gate name="-A" symbol="A16"/>
<gate name="-B" symbol="B16"/>
<gate name="-C" symbol="C16"/>
<gate name="-1" symbol="IO-44"/>
<gate name="-2" symbol="IO-84"/>
<gate name="-3" symbol="IO-124"/>
<gate name="-4" symbol="IO-164"/>
<gate name="-5" symbol="IO-204"/>
<gate name="-6" symbol="IO-244"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC40" symbol="NC"/>
<gate name="NC41" symbol="NC"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="FBGA256">
<connects>
<connect gate="-1" pin="IO11" pad="T2"/>
<connect gate="-1" pin="IO12" pad="T1"/>
<connect gate="-1" pin="IO13" pad="B3"/>
<connect gate="-1" pin="IO14" pad="A2"/>
<connect gate="-1" pin="IO21" pad="T3"/>
<connect gate="-1" pin="IO22" pad="C3"/>
<connect gate="-1" pin="IO23" pad="A3"/>
<connect gate="-1" pin="IO24" pad="R3"/>
<connect gate="-1" pin="IO31" pad="P4"/>
<connect gate="-1" pin="IO32" pad="P3"/>
<connect gate="-1" pin="IO33" pad="B4"/>
<connect gate="-1" pin="IO34" pad="A4"/>
<connect gate="-1" pin="IO41" pad="R4"/>
<connect gate="-1" pin="IO42" pad="C4"/>
<connect gate="-1" pin="IO43" pad="D4"/>
<connect gate="-1" pin="IO44" pad="T4"/>
<connect gate="-2" pin="IO51" pad="P5"/>
<connect gate="-2" pin="IO52" pad="N5"/>
<connect gate="-2" pin="IO53" pad="B5"/>
<connect gate="-2" pin="IO54" pad="A5"/>
<connect gate="-2" pin="IO61" pad="T5"/>
<connect gate="-2" pin="IO62" pad="C5"/>
<connect gate="-2" pin="IO63" pad="D5"/>
<connect gate="-2" pin="IO64" pad="R5"/>
<connect gate="-2" pin="IO71" pad="T6"/>
<connect gate="-2" pin="IO72" pad="N6"/>
<connect gate="-2" pin="IO73" pad="E4"/>
<connect gate="-2" pin="IO74" pad="B6"/>
<connect gate="-2" pin="IO81" pad="P6"/>
<connect gate="-2" pin="IO82" pad="R6"/>
<connect gate="-2" pin="IO83" pad="A6"/>
<connect gate="-2" pin="IO84" pad="C6"/>
<connect gate="-3" pin="IO101" pad="T7"/>
<connect gate="-3" pin="IO102" pad="R7"/>
<connect gate="-3" pin="IO103" pad="B7"/>
<connect gate="-3" pin="IO104" pad="C7"/>
<connect gate="-3" pin="IO111" pad="M8"/>
<connect gate="-3" pin="IO112" pad="P7"/>
<connect gate="-3" pin="IO113" pad="D7"/>
<connect gate="-3" pin="IO114" pad="E7"/>
<connect gate="-3" pin="IO121" pad="N8"/>
<connect gate="-3" pin="IO122" pad="C8"/>
<connect gate="-3" pin="IO123" pad="D8"/>
<connect gate="-3" pin="IO124" pad="P8"/>
<connect gate="-3" pin="IO91" pad="M7"/>
<connect gate="-3" pin="IO92" pad="D6"/>
<connect gate="-3" pin="IO93" pad="A7"/>
<connect gate="-3" pin="IO94" pad="N7"/>
<connect gate="-4" pin="IO131" pad="T9"/>
<connect gate="-4" pin="IO132" pad="P9"/>
<connect gate="-4" pin="IO133" pad="C9"/>
<connect gate="-4" pin="IO134" pad="D9"/>
<connect gate="-4" pin="IO141" pad="N9"/>
<connect gate="-4" pin="IO142" pad="R9"/>
<connect gate="-4" pin="IO143" pad="A10"/>
<connect gate="-4" pin="IO144" pad="E9"/>
<connect gate="-4" pin="IO151" pad="P10"/>
<connect gate="-4" pin="IO152" pad="B10"/>
<connect gate="-4" pin="IO153" pad="C10"/>
<connect gate="-4" pin="IO154" pad="R10"/>
<connect gate="-4" pin="IO161" pad="N10"/>
<connect gate="-4" pin="IO162" pad="T10"/>
<connect gate="-4" pin="IO163" pad="E10"/>
<connect gate="-4" pin="IO164" pad="D10"/>
<connect gate="-5" pin="IO171" pad="M10"/>
<connect gate="-5" pin="IO172" pad="A11"/>
<connect gate="-5" pin="IO173" pad="B11"/>
<connect gate="-5" pin="IO174" pad="N11"/>
<connect gate="-5" pin="IO181" pad="T11"/>
<connect gate="-5" pin="IO182" pad="R11"/>
<connect gate="-5" pin="IO183" pad="C11"/>
<connect gate="-5" pin="IO184" pad="D11"/>
<connect gate="-5" pin="IO191" pad="P12"/>
<connect gate="-5" pin="IO192" pad="R12"/>
<connect gate="-5" pin="IO193" pad="B12"/>
<connect gate="-5" pin="IO194" pad="A12"/>
<connect gate="-5" pin="IO201" pad="T13"/>
<connect gate="-5" pin="IO202" pad="C12"/>
<connect gate="-5" pin="IO203" pad="A13"/>
<connect gate="-5" pin="IO204" pad="T12"/>
<connect gate="-6" pin="IO211" pad="P13"/>
<connect gate="-6" pin="IO212" pad="R13"/>
<connect gate="-6" pin="IO213" pad="B13"/>
<connect gate="-6" pin="IO214" pad="D13"/>
<connect gate="-6" pin="IO221" pad="M13"/>
<connect gate="-6" pin="IO222" pad="N13"/>
<connect gate="-6" pin="IO223" pad="C14"/>
<connect gate="-6" pin="IO224" pad="C13"/>
<connect gate="-6" pin="IO231" pad="T15"/>
<connect gate="-6" pin="IO232" pad="A14"/>
<connect gate="-6" pin="IO233" pad="B14"/>
<connect gate="-6" pin="IO234" pad="T14"/>
<connect gate="-6" pin="IO241" pad="R15"/>
<connect gate="-6" pin="IO242" pad="R14"/>
<connect gate="-6" pin="IO243" pad="A15"/>
<connect gate="-6" pin="IO244" pad="A16"/>
<connect gate="-A" pin="IOA1" pad="D15"/>
<connect gate="-A" pin="IOA10" pad="C1"/>
<connect gate="-A" pin="IOA11" pad="F2"/>
<connect gate="-A" pin="IOA12" pad="F3"/>
<connect gate="-A" pin="IOA13" pad="F4"/>
<connect gate="-A" pin="IOA14" pad="E2"/>
<connect gate="-A" pin="IOA15" pad="D2"/>
<connect gate="-A" pin="IOA16" pad="D3"/>
<connect gate="-A" pin="IOA2" pad="F13"/>
<connect gate="-A" pin="IOA3" pad="G12"/>
<connect gate="-A" pin="IOA4" pad="G13"/>
<connect gate="-A" pin="IOA5" pad="G14"/>
<connect gate="-A" pin="IOA6" pad="H12"/>
<connect gate="-A" pin="IOA7" pad="G15"/>
<connect gate="-A" pin="IOA8" pad="G16"/>
<connect gate="-A" pin="IOA9" pad="G5"/>
<connect gate="-B" pin="IOB1" pad="H13"/>
<connect gate="-B" pin="IOB10" pad="H2"/>
<connect gate="-B" pin="IOB11" pad="G1"/>
<connect gate="-B" pin="IOB12" pad="H3"/>
<connect gate="-B" pin="IOB13" pad="H5"/>
<connect gate="-B" pin="IOB14" pad="G4"/>
<connect gate="-B" pin="IOB15" pad="G2"/>
<connect gate="-B" pin="IOB16" pad="F1"/>
<connect gate="-B" pin="IOB2" pad="H14"/>
<connect gate="-B" pin="IOB3" pad="H15"/>
<connect gate="-B" pin="IOB4" pad="J12"/>
<connect gate="-B" pin="IOB5" pad="J13"/>
<connect gate="-B" pin="IOB6" pad="J14"/>
<connect gate="-B" pin="IOB7" pad="J16"/>
<connect gate="-B" pin="IOB8" pad="J15"/>
<connect gate="-B" pin="IOB9" pad="J3"/>
<connect gate="-C" pin="IOC1" pad="K13"/>
<connect gate="-C" pin="IOC10" pad="L1"/>
<connect gate="-C" pin="IOC11" pad="L3"/>
<connect gate="-C" pin="IOC12" pad="K5"/>
<connect gate="-C" pin="IOC13" pad="K1"/>
<connect gate="-C" pin="IOC14" pad="K4"/>
<connect gate="-C" pin="IOC15" pad="J5"/>
<connect gate="-C" pin="IOC16" pad="J4"/>
<connect gate="-C" pin="IOC2" pad="L14"/>
<connect gate="-C" pin="IOC3" pad="L15"/>
<connect gate="-C" pin="IOC4" pad="L16"/>
<connect gate="-C" pin="IOC5" pad="N16"/>
<connect gate="-C" pin="IOC6" pad="L13"/>
<connect gate="-C" pin="IOC7" pad="P16"/>
<connect gate="-C" pin="IOC8" pad="M15"/>
<connect gate="-C" pin="IOC9" pad="M1"/>
<connect gate="G1" pin="GND" pad="E5"/>
<connect gate="G10" pin="GND" pad="J8"/>
<connect gate="G11" pin="GND" pad="J9"/>
<connect gate="G12" pin="GND" pad="K7"/>
<connect gate="G13" pin="GND" pad="K10"/>
<connect gate="G14" pin="GND" pad="L6"/>
<connect gate="G15" pin="GND" pad="L11"/>
<connect gate="G16" pin="GND" pad="M5"/>
<connect gate="G17" pin="GND" pad="M12"/>
<connect gate="G18" pin="GND" pad="T8"/>
<connect gate="G2" pin="GND" pad="E12"/>
<connect gate="G3" pin="GND" pad="F6"/>
<connect gate="G4" pin="GND" pad="F11"/>
<connect gate="G5" pin="GND" pad="G7"/>
<connect gate="G6" pin="GND" pad="G9"/>
<connect gate="G7" pin="GND" pad="G10"/>
<connect gate="G8" pin="GND" pad="H8"/>
<connect gate="G9" pin="GND" pad="H9"/>
<connect gate="NC1" pin="NC" pad="A8"/>
<connect gate="NC10" pin="NC" pad="E15"/>
<connect gate="NC11" pin="NC" pad="E16"/>
<connect gate="NC12" pin="NC" pad="F14"/>
<connect gate="NC13" pin="NC" pad="F15"/>
<connect gate="NC14" pin="NC" pad="F16"/>
<connect gate="NC15" pin="NC" pad="G3"/>
<connect gate="NC16" pin="NC" pad="H1"/>
<connect gate="NC17" pin="NC" pad="H4"/>
<connect gate="NC18" pin="NC" pad="H16"/>
<connect gate="NC19" pin="NC" pad="J1"/>
<connect gate="NC2" pin="NC" pad="B8"/>
<connect gate="NC20" pin="NC" pad="J2"/>
<connect gate="NC21" pin="NC" pad="K2"/>
<connect gate="NC22" pin="NC" pad="K3"/>
<connect gate="NC23" pin="NC" pad="K12"/>
<connect gate="NC24" pin="NC" pad="K14"/>
<connect gate="NC25" pin="NC" pad="K15"/>
<connect gate="NC26" pin="NC" pad="K16"/>
<connect gate="NC27" pin="NC" pad="L2"/>
<connect gate="NC28" pin="NC" pad="L4"/>
<connect gate="NC29" pin="NC" pad="M2"/>
<connect gate="NC3" pin="NC" pad="D1"/>
<connect gate="NC30" pin="NC" pad="M3"/>
<connect gate="NC31" pin="NC" pad="M4"/>
<connect gate="NC32" pin="NC" pad="M14"/>
<connect gate="NC33" pin="NC" pad="M16"/>
<connect gate="NC34" pin="NC" pad="N1"/>
<connect gate="NC35" pin="NC" pad="N2"/>
<connect gate="NC36" pin="NC" pad="N3"/>
<connect gate="NC37" pin="NC" pad="N14"/>
<connect gate="NC38" pin="NC" pad="N15"/>
<connect gate="NC39" pin="NC" pad="P2"/>
<connect gate="NC4" pin="NC" pad="D14"/>
<connect gate="NC40" pin="NC" pad="P11"/>
<connect gate="NC41" pin="NC" pad="P14"/>
<connect gate="NC5" pin="NC" pad="D16"/>
<connect gate="NC6" pin="NC" pad="E1"/>
<connect gate="NC7" pin="NC" pad="E3"/>
<connect gate="NC8" pin="NC" pad="E13"/>
<connect gate="NC9" pin="NC" pad="E14"/>
<connect gate="V1" pin="VCC" pad="E11"/>
<connect gate="V10" pin="VCC" pad="J10"/>
<connect gate="V11" pin="VCC" pad="J11"/>
<connect gate="V12" pin="VCC" pad="K9"/>
<connect gate="V13" pin="VCC" pad="L5"/>
<connect gate="V14" pin="VCC" pad="L7"/>
<connect gate="V15" pin="VCC" pad="L9"/>
<connect gate="V16" pin="VCC" pad="L12"/>
<connect gate="V17" pin="VCC" pad="M11"/>
<connect gate="V18" pin="VCC" pad="R2"/>
<connect gate="V2" pin="VCC" pad="F5"/>
<connect gate="V3" pin="VCC" pad="F7"/>
<connect gate="V4" pin="VCC" pad="F9"/>
<connect gate="V5" pin="VCC" pad="F12"/>
<connect gate="V6" pin="VCC" pad="H6"/>
<connect gate="V7" pin="VCC" pad="H7"/>
<connect gate="V8" pin="VCC" pad="H10"/>
<connect gate="V9" pin="VCC" pad="J7"/>
<connect gate="VO1" pin="VCCIO" pad="D12"/>
<connect gate="VO10" pin="VCCIO" pad="K6"/>
<connect gate="VO11" pin="VCCIO" pad="K8"/>
<connect gate="VO12" pin="VCCIO" pad="K11"/>
<connect gate="VO13" pin="VCCIO" pad="L10"/>
<connect gate="VO14" pin="VCCIO" pad="M6"/>
<connect gate="VO15" pin="VCCIO" pad="N12"/>
<connect gate="VO2" pin="VCCIO" pad="E6"/>
<connect gate="VO3" pin="VCCIO" pad="F8"/>
<connect gate="VO4" pin="VCCIO" pad="F10"/>
<connect gate="VO5" pin="VCCIO" pad="G6"/>
<connect gate="VO6" pin="VCCIO" pad="G8"/>
<connect gate="VO7" pin="VCCIO" pad="G11"/>
<connect gate="VO8" pin="VCCIO" pad="H11"/>
<connect gate="VO9" pin="VCCIO" pad="J6"/>
<connect gate="_1" pin="/CE" pad="B1"/>
<connect gate="_1" pin="/CEO" pad="B16"/>
<connect gate="_1" pin="/CONFIG" pad="N4"/>
<connect gate="_1" pin="/STATUS" pad="T16"/>
<connect gate="_1" pin="CONF_DONE" pad="C15"/>
<connect gate="_1" pin="DATA0" pad="A1"/>
<connect gate="_1" pin="DCLK" pad="B2"/>
<connect gate="_1" pin="GCLK0" pad="L8"/>
<connect gate="_1" pin="GCLK1" pad="A9"/>
<connect gate="_1" pin="IN0" pad="M9"/>
<connect gate="_1" pin="IN1" pad="R8"/>
<connect gate="_1" pin="IN2" pad="E8"/>
<connect gate="_1" pin="IN3" pad="B9"/>
<connect gate="_1" pin="MSEL0" pad="R1"/>
<connect gate="_1" pin="MSEL1" pad="P1"/>
<connect gate="_1" pin="TCK" pad="B15"/>
<connect gate="_1" pin="TDI" pad="C2"/>
<connect gate="_1" pin="TDO" pad="C16"/>
<connect gate="_1" pin="TMS" pad="P15"/>
<connect gate="_1" pin="TRST" pad="R16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K100A-BGA356" prefix="IC">
<description>&lt;b&gt;EPF10K100&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100B356C"/>
<gate name="-A" symbol="100A16"/>
<gate name="-B" symbol="100B16"/>
<gate name="-C" symbol="100C16"/>
<gate name="-D" symbol="100D16"/>
<gate name="-E" symbol="100E16"/>
<gate name="-F" symbol="100F15"/>
<gate name="-G" symbol="100G16"/>
<gate name="-H" symbol="100H16"/>
<gate name="-I" symbol="100I16"/>
<gate name="-J" symbol="100J15"/>
<gate name="-L" symbol="100L16"/>
<gate name="-1" symbol="100-113"/>
<gate name="-2" symbol="100-181"/>
<gate name="-3" symbol="100-242"/>
<gate name="-4" symbol="100-311"/>
<gate name="-5" symbol="100-402"/>
<gate name="-6" symbol="100-473"/>
<gate name="-7" symbol="100-524"/>
<gate name="-K" symbol="100K15"/>
<gate name="G1" symbol="GNDINT"/>
<gate name="G2" symbol="GNDINT"/>
<gate name="G3" symbol="GNDINT"/>
<gate name="G4" symbol="GNDINT"/>
<gate name="G5" symbol="GNDINT"/>
<gate name="G6" symbol="GNDINT"/>
<gate name="G7" symbol="GNDINT"/>
<gate name="G8" symbol="GNDINT"/>
<gate name="G9" symbol="GNDINT"/>
<gate name="G10" symbol="GNDINT"/>
<gate name="G11" symbol="GNDINT"/>
<gate name="G12" symbol="GNDINT"/>
<gate name="G13" symbol="GNDINT"/>
<gate name="G14" symbol="GNDINT"/>
<gate name="G15" symbol="GNDINT"/>
<gate name="G16" symbol="GNDINT"/>
<gate name="G17" symbol="GNDINT"/>
<gate name="G18" symbol="GNDINT"/>
<gate name="G19" symbol="GNDINT"/>
<gate name="G20" symbol="GNDINT"/>
<gate name="G21" symbol="GNDINT"/>
<gate name="G22" symbol="GNDINT"/>
<gate name="G23" symbol="GNDINT"/>
<gate name="G24" symbol="GNDINT"/>
<gate name="G25" symbol="GNDINT"/>
<gate name="G26" symbol="GNDINT"/>
<gate name="G27" symbol="GNDINT"/>
<gate name="G28" symbol="GNDINT"/>
<gate name="G29" symbol="GNDINT"/>
<gate name="G30" symbol="GNDINT"/>
<gate name="G31" symbol="GNDINT"/>
<gate name="G32" symbol="GNDINT"/>
<gate name="G33" symbol="GNDINT"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="BGA356">
<connects>
<connect gate="-1" pin="IO101" pad="AD5"/>
<connect gate="-1" pin="IO102" pad="B6"/>
<connect gate="-1" pin="IO11" pad="C3"/>
<connect gate="-1" pin="IO111" pad="AF2"/>
<connect gate="-1" pin="IO113" pad="A4"/>
<connect gate="-1" pin="IO21" pad="C4"/>
<connect gate="-1" pin="IO31" pad="C5"/>
<connect gate="-1" pin="IO32" pad="B2"/>
<connect gate="-1" pin="IO42" pad="B3"/>
<connect gate="-1" pin="IO51" pad="C6"/>
<connect gate="-1" pin="IO61" pad="B5"/>
<connect gate="-1" pin="IO71" pad="A3"/>
<connect gate="-1" pin="IO73" pad="AE3"/>
<connect gate="-1" pin="IO81" pad="C7"/>
<connect gate="-1" pin="IO91" pad="C8"/>
<connect gate="-1" pin="IO92" pad="AD4"/>
<connect gate="-2" pin="IO121" pad="AE4"/>
<connect gate="-2" pin="IO122" pad="AD6"/>
<connect gate="-2" pin="IO124" pad="A5"/>
<connect gate="-2" pin="IO131" pad="B8"/>
<connect gate="-2" pin="IO132" pad="AE5"/>
<connect gate="-2" pin="IO141" pad="B7"/>
<connect gate="-2" pin="IO142" pad="AD7"/>
<connect gate="-2" pin="IO143" pad="AD8"/>
<connect gate="-2" pin="IO151" pad="C10"/>
<connect gate="-2" pin="IO152" pad="AF4"/>
<connect gate="-2" pin="IO162" pad="AD9"/>
<connect gate="-2" pin="IO163" pad="B9"/>
<connect gate="-2" pin="IO164" pad="AE6"/>
<connect gate="-2" pin="IO171" pad="AE8"/>
<connect gate="-2" pin="IO172" pad="A6"/>
<connect gate="-2" pin="IO181" pad="C11"/>
<connect gate="-3" pin="IO182" pad="AF5"/>
<connect gate="-3" pin="IO191" pad="B10"/>
<connect gate="-3" pin="IO192" pad="AE9"/>
<connect gate="-3" pin="IO194" pad="AD10"/>
<connect gate="-3" pin="IO201" pad="AF6"/>
<connect gate="-3" pin="IO202" pad="A8"/>
<connect gate="-3" pin="IO211" pad="B11"/>
<connect gate="-3" pin="IO212" pad="AE10"/>
<connect gate="-3" pin="IO221" pad="AD11"/>
<connect gate="-3" pin="IO222" pad="AF8"/>
<connect gate="-3" pin="IO223" pad="A9"/>
<connect gate="-3" pin="IO231" pad="C12"/>
<connect gate="-3" pin="IO232" pad="AE11"/>
<connect gate="-3" pin="IO234" pad="AF9"/>
<connect gate="-3" pin="IO241" pad="A11"/>
<connect gate="-3" pin="IO242" pad="AF10"/>
<connect gate="-4" pin="IO251" pad="B12"/>
<connect gate="-4" pin="IO252" pad="AE12"/>
<connect gate="-4" pin="IO253" pad="AD12"/>
<connect gate="-4" pin="IO261" pad="AD13"/>
<connect gate="-4" pin="IO263" pad="AF12"/>
<connect gate="-4" pin="IO264" pad="A12"/>
<connect gate="-4" pin="IO271" pad="A15"/>
<connect gate="-4" pin="IO272" pad="AE14"/>
<connect gate="-4" pin="IO281" pad="B15"/>
<connect gate="-4" pin="IO282" pad="AF15"/>
<connect gate="-4" pin="IO284" pad="AE15"/>
<connect gate="-4" pin="IO291" pad="A16"/>
<connect gate="-4" pin="IO294" pad="AD15"/>
<connect gate="-4" pin="IO301" pad="A17"/>
<connect gate="-4" pin="IO302" pad="AF17"/>
<connect gate="-4" pin="IO311" pad="B16"/>
<connect gate="-5" pin="IO321" pad="A18"/>
<connect gate="-5" pin="IO323" pad="AE16"/>
<connect gate="-5" pin="IO331" pad="B17"/>
<connect gate="-5" pin="IO333" pad="AF18"/>
<connect gate="-5" pin="IO341" pad="C16"/>
<connect gate="-5" pin="IO351" pad="A19"/>
<connect gate="-5" pin="IO353" pad="AE17"/>
<connect gate="-5" pin="IO361" pad="C18"/>
<connect gate="-5" pin="IO364" pad="AD16"/>
<connect gate="-5" pin="IO371" pad="AF20"/>
<connect gate="-5" pin="IO372" pad="B18"/>
<connect gate="-5" pin="IO381" pad="AE18"/>
<connect gate="-5" pin="IO391" pad="AD17"/>
<connect gate="-5" pin="IO392" pad="C17"/>
<connect gate="-5" pin="IO401" pad="A22"/>
<connect gate="-5" pin="IO402" pad="A21"/>
<connect gate="-6" pin="IO404" pad="AF21"/>
<connect gate="-6" pin="IO411" pad="AF22"/>
<connect gate="-6" pin="IO413" pad="B19"/>
<connect gate="-6" pin="IO414" pad="B20"/>
<connect gate="-6" pin="IO421" pad="A24"/>
<connect gate="-6" pin="IO423" pad="AE19"/>
<connect gate="-6" pin="IO431" pad="C19"/>
<connect gate="-6" pin="IO432" pad="AF23"/>
<connect gate="-6" pin="IO441" pad="AE20"/>
<connect gate="-6" pin="IO443" pad="B21"/>
<connect gate="-6" pin="IO451" pad="A25"/>
<connect gate="-6" pin="IO452" pad="AE21"/>
<connect gate="-6" pin="IO461" pad="AD19"/>
<connect gate="-6" pin="IO462" pad="C20"/>
<connect gate="-6" pin="IO471" pad="AF24"/>
<connect gate="-6" pin="IO473" pad="B23"/>
<connect gate="-7" pin="IO481" pad="C21"/>
<connect gate="-7" pin="IO482" pad="AE22"/>
<connect gate="-7" pin="IO491" pad="AE23"/>
<connect gate="-7" pin="IO492" pad="B24"/>
<connect gate="-7" pin="IO501" pad="AD21"/>
<connect gate="-7" pin="IO502" pad="AE24"/>
<connect gate="-7" pin="IO504" pad="C23"/>
<connect gate="-7" pin="IO511" pad="C22"/>
<connect gate="-7" pin="IO512" pad="AD23"/>
<connect gate="-7" pin="IO521" pad="C24"/>
<connect gate="-7" pin="IO522" pad="AD24"/>
<connect gate="-7" pin="IO524" pad="AD22"/>
<connect gate="-A" pin="IOA1" pad="AC26"/>
<connect gate="-A" pin="IOA10" pad="AB24"/>
<connect gate="-A" pin="IOA12" pad="AC4"/>
<connect gate="-A" pin="IOA14" pad="AB3"/>
<connect gate="-A" pin="IOA15" pad="AB25"/>
<connect gate="-A" pin="IOA16" pad="AB26"/>
<connect gate="-A" pin="IOA2" pad="AB22"/>
<connect gate="-A" pin="IOA3" pad="AB23"/>
<connect gate="-A" pin="IOA4" pad="AA24"/>
<connect gate="-A" pin="IOA5" pad="AB4"/>
<connect gate="-A" pin="IOA6" pad="AC1"/>
<connect gate="-A" pin="IOA7" pad="AD1"/>
<connect gate="-A" pin="IOA8" pad="AB5"/>
<connect gate="-A" pin="IOA9" pad="AB2"/>
<connect gate="-B" pin="IOB1" pad="AA22"/>
<connect gate="-B" pin="IOB10" pad="AA23"/>
<connect gate="-B" pin="IOB12" pad="Y22"/>
<connect gate="-B" pin="IOB16" pad="AA26"/>
<connect gate="-B" pin="IOB2" pad="AA25"/>
<connect gate="-B" pin="IOB3" pad="Y23"/>
<connect gate="-B" pin="IOB4" pad="Y4"/>
<connect gate="-B" pin="IOB5" pad="AA2"/>
<connect gate="-B" pin="IOB6" pad="Y5"/>
<connect gate="-B" pin="IOB7" pad="AA5"/>
<connect gate="-B" pin="IOB8" pad="AA4"/>
<connect gate="-B" pin="IOB9" pad="AA3"/>
<connect gate="-C" pin="IOC1" pad="Y26"/>
<connect gate="-C" pin="IOC10" pad="W3"/>
<connect gate="-C" pin="IOC11" pad="Y24"/>
<connect gate="-C" pin="IOC12" pad="W5"/>
<connect gate="-C" pin="IOC13" pad="W24"/>
<connect gate="-C" pin="IOC15" pad="V22"/>
<connect gate="-C" pin="IOC16" pad="W23"/>
<connect gate="-C" pin="IOC2" pad="W25"/>
<connect gate="-C" pin="IOC3" pad="W2"/>
<connect gate="-C" pin="IOC4" pad="Y1"/>
<connect gate="-C" pin="IOC5" pad="Y2"/>
<connect gate="-C" pin="IOC6" pad="Y3"/>
<connect gate="-C" pin="IOC8" pad="W4"/>
<connect gate="-C" pin="IOC9" pad="Y25"/>
<connect gate="-D" pin="IOD1" pad="U22"/>
<connect gate="-D" pin="IOD10" pad="V3"/>
<connect gate="-D" pin="IOD12" pad="V4"/>
<connect gate="-D" pin="IOD14" pad="V24"/>
<connect gate="-D" pin="IOD15" pad="U2"/>
<connect gate="-D" pin="IOD16" pad="U23"/>
<connect gate="-D" pin="IOD2" pad="W26"/>
<connect gate="-D" pin="IOD3" pad="V25"/>
<connect gate="-D" pin="IOD4" pad="T24"/>
<connect gate="-D" pin="IOD5" pad="U3"/>
<connect gate="-D" pin="IOD6" pad="U4"/>
<connect gate="-D" pin="IOD7" pad="V5"/>
<connect gate="-D" pin="IOD8" pad="V1"/>
<connect gate="-D" pin="IOD9" pad="V23"/>
<connect gate="-E" pin="IOE1" pad="U24"/>
<connect gate="-E" pin="IOE11" pad="V26"/>
<connect gate="-E" pin="IOE13" pad="R3"/>
<connect gate="-E" pin="IOE14" pad="U25"/>
<connect gate="-E" pin="IOE16" pad="T23"/>
<connect gate="-E" pin="IOE2" pad="T22"/>
<connect gate="-E" pin="IOE3" pad="T2"/>
<connect gate="-E" pin="IOE4" pad="T3"/>
<connect gate="-E" pin="IOE5" pad="U1"/>
<connect gate="-E" pin="IOE6" pad="R22"/>
<connect gate="-E" pin="IOE8" pad="T5"/>
<connect gate="-E" pin="IOE9" pad="T4"/>
<connect gate="-F" pin="IOF1" pad="R25"/>
<connect gate="-F" pin="IOF11" pad="P22"/>
<connect gate="-F" pin="IOF12" pad="P25"/>
<connect gate="-F" pin="IOF13" pad="R4"/>
<connect gate="-F" pin="IOF14" pad="R5"/>
<connect gate="-F" pin="IOF15" pad="P1"/>
<connect gate="-F" pin="IOF2" pad="P23"/>
<connect gate="-F" pin="IOF3" pad="P5"/>
<connect gate="-F" pin="IOF4" pad="P3"/>
<connect gate="-F" pin="IOF5" pad="R2"/>
<connect gate="-F" pin="IOF6" pad="R24"/>
<connect gate="-F" pin="IOF7" pad="R23"/>
<connect gate="-F" pin="IOF8" pad="P4"/>
<connect gate="-F" pin="IOF9" pad="P24"/>
<connect gate="-G" pin="IOG1" pad="N23"/>
<connect gate="-G" pin="IOG10" pad="P26"/>
<connect gate="-G" pin="IOG11" pad="N25"/>
<connect gate="-G" pin="IOG12" pad="N22"/>
<connect gate="-G" pin="IOG13" pad="M5"/>
<connect gate="-G" pin="IOG15" pad="M25"/>
<connect gate="-G" pin="IOG16" pad="M24"/>
<connect gate="-G" pin="IOG2" pad="N24"/>
<connect gate="-G" pin="IOG3" pad="N2"/>
<connect gate="-G" pin="IOG4" pad="N3"/>
<connect gate="-G" pin="IOG5" pad="N5"/>
<connect gate="-G" pin="IOG6" pad="N4"/>
<connect gate="-G" pin="IOG8" pad="M3"/>
<connect gate="-G" pin="IOG9" pad="M2"/>
<connect gate="-H" pin="IOH1" pad="L26"/>
<connect gate="-H" pin="IOH11" pad="L5"/>
<connect gate="-H" pin="IOH12" pad="M22"/>
<connect gate="-H" pin="IOH13" pad="L24"/>
<connect gate="-H" pin="IOH14" pad="L4"/>
<connect gate="-H" pin="IOH16" pad="L23"/>
<connect gate="-H" pin="IOH2" pad="L22"/>
<connect gate="-H" pin="IOH3" pad="L25"/>
<connect gate="-H" pin="IOH4" pad="K2"/>
<connect gate="-H" pin="IOH5" pad="M4"/>
<connect gate="-H" pin="IOH7" pad="L2"/>
<connect gate="-H" pin="IOH8" pad="L1"/>
<connect gate="-I" pin="IOI1" pad="K24"/>
<connect gate="-I" pin="IOI10" pad="K25"/>
<connect gate="-I" pin="IOI12" pad="J24"/>
<connect gate="-I" pin="IOI13" pad="J5"/>
<connect gate="-I" pin="IOI14" pad="K22"/>
<connect gate="-I" pin="IOI15" pad="K26"/>
<connect gate="-I" pin="IOI16" pad="J25"/>
<connect gate="-I" pin="IOI2" pad="K23"/>
<connect gate="-I" pin="IOI3" pad="J2"/>
<connect gate="-I" pin="IOI4" pad="L3"/>
<connect gate="-I" pin="IOI5" pad="K4"/>
<connect gate="-I" pin="IOI6" pad="K3"/>
<connect gate="-I" pin="IOI7" pad="J4"/>
<connect gate="-I" pin="IOI9" pad="J3"/>
<connect gate="-J" pin="IOJ1" pad="H26"/>
<connect gate="-J" pin="IOJ10" pad="G26"/>
<connect gate="-J" pin="IOJ11" pad="G3"/>
<connect gate="-J" pin="IOJ12" pad="H5"/>
<connect gate="-J" pin="IOJ13" pad="J22"/>
<connect gate="-J" pin="IOJ14" pad="G2"/>
<connect gate="-J" pin="IOJ15" pad="G24"/>
<connect gate="-J" pin="IOJ2" pad="G25"/>
<connect gate="-J" pin="IOJ3" pad="H1"/>
<connect gate="-J" pin="IOJ5" pad="H2"/>
<connect gate="-J" pin="IOJ6" pad="H4"/>
<connect gate="-J" pin="IOJ7" pad="H25"/>
<connect gate="-J" pin="IOJ8" pad="H3"/>
<connect gate="-J" pin="IOJ9" pad="J23"/>
<connect gate="-K" pin="IOK1" pad="F25"/>
<connect gate="-K" pin="IOK10" pad="G1"/>
<connect gate="-K" pin="IOK11" pad="G22"/>
<connect gate="-K" pin="IOK14" pad="F5"/>
<connect gate="-K" pin="IOK15" pad="F24"/>
<connect gate="-K" pin="IOK2" pad="F22"/>
<connect gate="-K" pin="IOK3" pad="F2"/>
<connect gate="-K" pin="IOK4" pad="G4"/>
<connect gate="-K" pin="IOK5" pad="G5"/>
<connect gate="-K" pin="IOK6" pad="G23"/>
<connect gate="-K" pin="IOK7" pad="F26"/>
<connect gate="-K" pin="IOK8" pad="F3"/>
<connect gate="-L" pin="IOL1" pad="E25"/>
<connect gate="-L" pin="IOL10" pad="F23"/>
<connect gate="-L" pin="IOL11" pad="E2"/>
<connect gate="-L" pin="IOL12" pad="E26"/>
<connect gate="-L" pin="IOL13" pad="C1"/>
<connect gate="-L" pin="IOL15" pad="E23"/>
<connect gate="-L" pin="IOL16" pad="E22"/>
<connect gate="-L" pin="IOL2" pad="E24"/>
<connect gate="-L" pin="IOL3" pad="D26"/>
<connect gate="-L" pin="IOL4" pad="E3"/>
<connect gate="-L" pin="IOL5" pad="E4"/>
<connect gate="-L" pin="IOL6" pad="E1"/>
<connect gate="-L" pin="IOL7" pad="D1"/>
<connect gate="-L" pin="IOL8" pad="E5"/>
<connect gate="G1" pin="GND" pad="AD2"/>
<connect gate="G10" pin="GND" pad="AF19"/>
<connect gate="G11" pin="GND" pad="AF25"/>
<connect gate="G12" pin="GND" pad="A2"/>
<connect gate="G13" pin="GND" pad="A10"/>
<connect gate="G14" pin="GND" pad="A20"/>
<connect gate="G15" pin="GND" pad="B1"/>
<connect gate="G16" pin="GND" pad="B13"/>
<connect gate="G17" pin="GND" pad="B22"/>
<connect gate="G18" pin="GND" pad="B25"/>
<connect gate="G19" pin="GND" pad="B26"/>
<connect gate="G2" pin="GND" pad="AD14"/>
<connect gate="G20" pin="GND" pad="C2"/>
<connect gate="G21" pin="GND" pad="C9"/>
<connect gate="G22" pin="GND" pad="C13"/>
<connect gate="G23" pin="GND" pad="C25"/>
<connect gate="G24" pin="GND" pad="H23"/>
<connect gate="G25" pin="GND" pad="J26"/>
<connect gate="G26" pin="GND" pad="K1"/>
<connect gate="G27" pin="GND" pad="M1"/>
<connect gate="G28" pin="GND" pad="N26"/>
<connect gate="G29" pin="GND" pad="R1"/>
<connect gate="G3" pin="GND" pad="AD20"/>
<connect gate="G30" pin="GND" pad="R26"/>
<connect gate="G31" pin="GND" pad="T1"/>
<connect gate="G32" pin="GND" pad="U26"/>
<connect gate="G33" pin="GND" pad="W1"/>
<connect gate="G4" pin="GND" pad="AE1"/>
<connect gate="G5" pin="GND" pad="AE2"/>
<connect gate="G6" pin="GND" pad="AE7"/>
<connect gate="G7" pin="GND" pad="AE25"/>
<connect gate="G8" pin="GND" pad="AE26"/>
<connect gate="G9" pin="GND" pad="AF11"/>
<connect gate="V1" pin="VCC" pad="AA1"/>
<connect gate="V10" pin="VCC" pad="H22"/>
<connect gate="V11" pin="VCC" pad="J1"/>
<connect gate="V12" pin="VCC" pad="M26"/>
<connect gate="V13" pin="VCC" pad="N1"/>
<connect gate="V14" pin="VCC" pad="T26"/>
<connect gate="V15" pin="VCC" pad="U5"/>
<connect gate="V2" pin="VCC" pad="AD26"/>
<connect gate="V3" pin="VCC" pad="AF1"/>
<connect gate="V4" pin="VCC" pad="AF26"/>
<connect gate="V5" pin="VCC" pad="A1"/>
<connect gate="V6" pin="VCC" pad="A26"/>
<connect gate="V7" pin="VCC" pad="C14"/>
<connect gate="V8" pin="VCC" pad="C26"/>
<connect gate="V9" pin="VCC" pad="D5"/>
<connect gate="VO1" pin="VCCIO" pad="AB1"/>
<connect gate="VO10" pin="VCCIO" pad="C15"/>
<connect gate="VO11" pin="VCCIO" pad="D25"/>
<connect gate="VO12" pin="VCCIO" pad="F4"/>
<connect gate="VO13" pin="VCCIO" pad="H24"/>
<connect gate="VO14" pin="VCCIO" pad="K5"/>
<connect gate="VO15" pin="VCCIO" pad="M23"/>
<connect gate="VO16" pin="VCCIO" pad="P2"/>
<connect gate="VO17" pin="VCCIO" pad="T25"/>
<connect gate="VO18" pin="VCCIO" pad="V2"/>
<connect gate="VO19" pin="VCCIO" pad="W22"/>
<connect gate="VO2" pin="VCCIO" pad="AC25"/>
<connect gate="VO3" pin="VCCIO" pad="AD18"/>
<connect gate="VO4" pin="VCCIO" pad="AF3"/>
<connect gate="VO5" pin="VCCIO" pad="AF7"/>
<connect gate="VO6" pin="VCCIO" pad="AF16"/>
<connect gate="VO7" pin="VCCIO" pad="A7"/>
<connect gate="VO8" pin="VCCIO" pad="A23"/>
<connect gate="VO9" pin="VCCIO" pad="B4"/>
<connect gate="_" pin="/CE" pad="AC2"/>
<connect gate="_" pin="/CEO" pad="AC22"/>
<connect gate="_" pin="/CONFIG" pad="D2"/>
<connect gate="_" pin="/STATUS" pad="D24"/>
<connect gate="_" pin="CONF_DONE" pad="AC24"/>
<connect gate="_" pin="DATA0" pad="AD3"/>
<connect gate="_" pin="DCLK" pad="AC5"/>
<connect gate="_" pin="GCLK" pad="AF13"/>
<connect gate="_" pin="GCLK1" pad="A14"/>
<connect gate="_" pin="IN0" pad="B14"/>
<connect gate="_" pin="IN1" pad="A13"/>
<connect gate="_" pin="IN2" pad="AE13"/>
<connect gate="_" pin="IN3" pad="AF14"/>
<connect gate="_" pin="MSEL0" pad="D4"/>
<connect gate="_" pin="MSEL1" pad="D3"/>
<connect gate="_" pin="TCK" pad="AD25"/>
<connect gate="_" pin="TDI" pad="AC3"/>
<connect gate="_" pin="TDO" pad="AC23"/>
<connect gate="_" pin="TMS" pad="D22"/>
<connect gate="_" pin="TRST" pad="D23"/>
<connect gate="_" pin="VCC_CKLK" pad="F1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K100ABC356-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8777"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K100A-FBGA484" prefix="IC">
<description>&lt;b&gt;EPF10K100&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100B484C"/>
<gate name="-A" symbol="A484"/>
<gate name="-B" symbol="B484"/>
<gate name="-C" symbol="C484"/>
<gate name="-D" symbol="D484"/>
<gate name="-E" symbol="E484"/>
<gate name="-F" symbol="F484"/>
<gate name="-G" symbol="G484"/>
<gate name="-H" symbol="H484"/>
<gate name="-I" symbol="I484"/>
<gate name="-J" symbol="J484"/>
<gate name="-K" symbol="K484"/>
<gate name="-L" symbol="L484"/>
<gate name="-1" symbol="IO51"/>
<gate name="-2" symbol="IO92"/>
<gate name="-3" symbol="IO133"/>
<gate name="-4" symbol="IO173"/>
<gate name="-5" symbol="IO214"/>
<gate name="-6" symbol="IO254"/>
<gate name="-7" symbol="IO302"/>
<gate name="-8" symbol="IO353"/>
<gate name="-9" symbol="IO401"/>
<gate name="-10" symbol="IO443"/>
<gate name="-11" symbol="IO483"/>
<gate name="-12" symbol="IO524"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="FBGA484">
<connects>
<connect gate="-1" pin="IO11" pad="AA2"/>
<connect gate="-1" pin="IO12" pad="B10"/>
<connect gate="-1" pin="IO13" pad="W4"/>
<connect gate="-1" pin="IO14" pad="A2"/>
<connect gate="-1" pin="IO21" pad="Y4"/>
<connect gate="-1" pin="IO22" pad="W5"/>
<connect gate="-1" pin="IO23" pad="B3"/>
<connect gate="-1" pin="IO24" pad="B4"/>
<connect gate="-1" pin="IO31" pad="Y5"/>
<connect gate="-1" pin="IO32" pad="U7"/>
<connect gate="-1" pin="IO33" pad="A3"/>
<connect gate="-1" pin="IO34" pad="A5"/>
<connect gate="-1" pin="IO41" pad="AA3"/>
<connect gate="-1" pin="IO42" pad="W3"/>
<connect gate="-1" pin="IO44" pad="A4"/>
<connect gate="-1" pin="IO51" pad="AB1"/>
<connect gate="-10" pin="IO402" pad="V16"/>
<connect gate="-10" pin="IO404" pad="E15"/>
<connect gate="-10" pin="IO411" pad="E16"/>
<connect gate="-10" pin="IO412" pad="B16"/>
<connect gate="-10" pin="IO413" pad="AA16"/>
<connect gate="-10" pin="IO414" pad="W16"/>
<connect gate="-10" pin="IO421" pad="V17"/>
<connect gate="-10" pin="IO423" pad="D16"/>
<connect gate="-10" pin="IO424" pad="C16"/>
<connect gate="-10" pin="IO431" pad="W17"/>
<connect gate="-10" pin="IO432" pad="A16"/>
<connect gate="-10" pin="IO433" pad="Y16"/>
<connect gate="-10" pin="IO434" pad="A17"/>
<connect gate="-10" pin="IO441" pad="A18"/>
<connect gate="-10" pin="IO442" pad="AB17"/>
<connect gate="-10" pin="IO443" pad="Y17"/>
<connect gate="-11" pin="IO444" pad="C17"/>
<connect gate="-11" pin="IO451" pad="AA17"/>
<connect gate="-11" pin="IO452" pad="A19"/>
<connect gate="-11" pin="IO453" pad="V18"/>
<connect gate="-11" pin="IO454" pad="D20"/>
<connect gate="-11" pin="IO461" pad="B18"/>
<connect gate="-11" pin="IO462" pad="U17"/>
<connect gate="-11" pin="IO463" pad="AB18"/>
<connect gate="-11" pin="IO464" pad="C20"/>
<connect gate="-11" pin="IO471" pad="A20"/>
<connect gate="-11" pin="IO472" pad="AB19"/>
<connect gate="-11" pin="IO473" pad="W18"/>
<connect gate="-11" pin="IO474" pad="D17"/>
<connect gate="-11" pin="IO481" pad="AA18"/>
<connect gate="-11" pin="IO482" pad="C18"/>
<connect gate="-11" pin="IO483" pad="AB20"/>
<connect gate="-12" pin="IO491" pad="F17"/>
<connect gate="-12" pin="IO492" pad="AA19"/>
<connect gate="-12" pin="IO493" pad="Y18"/>
<connect gate="-12" pin="IO494" pad="B19"/>
<connect gate="-12" pin="IO501" pad="A21"/>
<connect gate="-12" pin="IO502" pad="E17"/>
<connect gate="-12" pin="IO503" pad="Y19"/>
<connect gate="-12" pin="IO504" pad="AB21"/>
<connect gate="-12" pin="IO511" pad="AA20"/>
<connect gate="-12" pin="IO512" pad="D18"/>
<connect gate="-12" pin="IO513" pad="AA21"/>
<connect gate="-12" pin="IO514" pad="B20"/>
<connect gate="-12" pin="IO521" pad="AB22"/>
<connect gate="-12" pin="IO522" pad="D19"/>
<connect gate="-12" pin="IO523" pad="Y20"/>
<connect gate="-12" pin="IO524" pad="C19"/>
<connect gate="-2" pin="IO52" pad="AB2"/>
<connect gate="-2" pin="IO53" pad="F7"/>
<connect gate="-2" pin="IO61" pad="W6"/>
<connect gate="-2" pin="IO62" pad="AA4"/>
<connect gate="-2" pin="IO63" pad="C5"/>
<connect gate="-2" pin="IO64" pad="D6"/>
<connect gate="-2" pin="IO71" pad="V7"/>
<connect gate="-2" pin="IO72" pad="AA5"/>
<connect gate="-2" pin="IO73" pad="C6"/>
<connect gate="-2" pin="IO74" pad="C4"/>
<connect gate="-2" pin="IO81" pad="Y6"/>
<connect gate="-2" pin="IO82" pad="U8"/>
<connect gate="-2" pin="IO83" pad="B6"/>
<connect gate="-2" pin="IO84" pad="C3"/>
<connect gate="-2" pin="IO91" pad="V8"/>
<connect gate="-2" pin="IO92" pad="E6"/>
<connect gate="-3" pin="IO101" pad="D5"/>
<connect gate="-3" pin="IO102" pad="W7"/>
<connect gate="-3" pin="IO103" pad="C7"/>
<connect gate="-3" pin="IO104" pad="AB4"/>
<connect gate="-3" pin="IO111" pad="F6"/>
<connect gate="-3" pin="IO112" pad="AB5"/>
<connect gate="-3" pin="IO113" pad="AB6"/>
<connect gate="-3" pin="IO121" pad="A7"/>
<connect gate="-3" pin="IO122" pad="E7"/>
<connect gate="-3" pin="IO123" pad="AA7"/>
<connect gate="-3" pin="IO124" pad="Y7"/>
<connect gate="-3" pin="IO131" pad="W8"/>
<connect gate="-3" pin="IO132" pad="D7"/>
<connect gate="-3" pin="IO133" pad="AB7"/>
<connect gate="-3" pin="IO93" pad="AB3"/>
<connect gate="-3" pin="IO94" pad="F8"/>
<connect gate="-4" pin="IO134" pad="B7"/>
<connect gate="-4" pin="IO141" pad="U9"/>
<connect gate="-4" pin="IO142" pad="D8"/>
<connect gate="-4" pin="IO143" pad="G7"/>
<connect gate="-4" pin="IO144" pad="V9"/>
<connect gate="-4" pin="IO151" pad="AB8"/>
<connect gate="-4" pin="IO152" pad="E8"/>
<connect gate="-4" pin="IO153" pad="AA8"/>
<connect gate="-4" pin="IO154" pad="C8"/>
<connect gate="-4" pin="IO161" pad="R10"/>
<connect gate="-4" pin="IO162" pad="G9"/>
<connect gate="-4" pin="IO163" pad="T10"/>
<connect gate="-4" pin="IO164" pad="B8"/>
<connect gate="-4" pin="IO171" pad="G8"/>
<connect gate="-4" pin="IO172" pad="Y9"/>
<connect gate="-4" pin="IO173" pad="R11"/>
<connect gate="-5" pin="IO174" pad="F9"/>
<connect gate="-5" pin="IO181" pad="AA9"/>
<connect gate="-5" pin="IO182" pad="C9"/>
<connect gate="-5" pin="IO183" pad="W9"/>
<connect gate="-5" pin="IO184" pad="D9"/>
<connect gate="-5" pin="IO191" pad="AB9"/>
<connect gate="-5" pin="IO192" pad="B9"/>
<connect gate="-5" pin="IO194" pad="A9"/>
<connect gate="-5" pin="IO201" pad="E9"/>
<connect gate="-5" pin="IO202" pad="V10"/>
<connect gate="-5" pin="IO203" pad="U10"/>
<connect gate="-5" pin="IO204" pad="H10"/>
<connect gate="-5" pin="IO211" pad="Y10"/>
<connect gate="-5" pin="IO212" pad="C10"/>
<connect gate="-5" pin="IO213" pad="T11"/>
<connect gate="-5" pin="IO214" pad="F10"/>
<connect gate="-6" pin="IO221" pad="D10"/>
<connect gate="-6" pin="IO222" pad="E10"/>
<connect gate="-6" pin="IO223" pad="AA10"/>
<connect gate="-6" pin="IO224" pad="W10"/>
<connect gate="-6" pin="IO231" pad="AB10"/>
<connect gate="-6" pin="IO232" pad="F11"/>
<connect gate="-6" pin="IO233" pad="T12"/>
<connect gate="-6" pin="IO234" pad="A10"/>
<connect gate="-6" pin="IO241" pad="U11"/>
<connect gate="-6" pin="IO242" pad="E11"/>
<connect gate="-6" pin="IO243" pad="U12"/>
<connect gate="-6" pin="IO244" pad="G10"/>
<connect gate="-6" pin="IO251" pad="Y11"/>
<connect gate="-6" pin="IO252" pad="B11"/>
<connect gate="-6" pin="IO253" pad="D11"/>
<connect gate="-6" pin="IO254" pad="V12"/>
<connect gate="-7" pin="IO261" pad="G11"/>
<connect gate="-7" pin="IO263" pad="A11"/>
<connect gate="-7" pin="IO264" pad="AA11"/>
<connect gate="-7" pin="IO271" pad="AB12"/>
<connect gate="-7" pin="IO272" pad="F12"/>
<connect gate="-7" pin="IO273" pad="W12"/>
<connect gate="-7" pin="IO274" pad="C12"/>
<connect gate="-7" pin="IO281" pad="R13"/>
<connect gate="-7" pin="IO282" pad="B12"/>
<connect gate="-7" pin="IO283" pad="Y12"/>
<connect gate="-7" pin="IO284" pad="A12"/>
<connect gate="-7" pin="IO291" pad="V13"/>
<connect gate="-7" pin="IO293" pad="U13"/>
<connect gate="-7" pin="IO294" pad="G12"/>
<connect gate="-7" pin="IO301" pad="W13"/>
<connect gate="-7" pin="IO302" pad="H12"/>
<connect gate="-8" pin="IO303" pad="T13"/>
<connect gate="-8" pin="IO311" pad="Y13"/>
<connect gate="-8" pin="IO312" pad="C13"/>
<connect gate="-8" pin="IO313" pad="AA13"/>
<connect gate="-8" pin="IO321" pad="T14"/>
<connect gate="-8" pin="IO322" pad="V14"/>
<connect gate="-8" pin="IO323" pad="B13"/>
<connect gate="-8" pin="IO331" pad="AB14"/>
<connect gate="-8" pin="IO332" pad="W14"/>
<connect gate="-8" pin="IO333" pad="D13"/>
<connect gate="-8" pin="IO341" pad="AA14"/>
<connect gate="-8" pin="IO343" pad="F13"/>
<connect gate="-8" pin="IO344" pad="E13"/>
<connect gate="-8" pin="IO351" pad="U14"/>
<connect gate="-8" pin="IO352" pad="Y14"/>
<connect gate="-8" pin="IO353" pad="D14"/>
<connect gate="-9" pin="IO354" pad="C14"/>
<connect gate="-9" pin="IO361" pad="U15"/>
<connect gate="-9" pin="IO362" pad="W15"/>
<connect gate="-9" pin="IO363" pad="A14"/>
<connect gate="-9" pin="IO364" pad="B14"/>
<connect gate="-9" pin="IO371" pad="B15"/>
<connect gate="-9" pin="IO372" pad="V15"/>
<connect gate="-9" pin="IO373" pad="AB15"/>
<connect gate="-9" pin="IO374" pad="E14"/>
<connect gate="-9" pin="IO381" pad="A15"/>
<connect gate="-9" pin="IO383" pad="Y15"/>
<connect gate="-9" pin="IO384" pad="F14"/>
<connect gate="-9" pin="IO391" pad="D15"/>
<connect gate="-9" pin="IO392" pad="T16"/>
<connect gate="-9" pin="IO394" pad="AA15"/>
<connect gate="-9" pin="IO401" pad="U16"/>
<connect gate="-A" pin="IOA1" pad="C22"/>
<connect gate="-A" pin="IOA10" pad="D22"/>
<connect gate="-A" pin="IOA12" pad="D3"/>
<connect gate="-A" pin="IOA14" pad="F1"/>
<connect gate="-A" pin="IOA15" pad="E22"/>
<connect gate="-A" pin="IOA16" pad="F20"/>
<connect gate="-A" pin="IOA2" pad="D21"/>
<connect gate="-A" pin="IOA3" pad="E20"/>
<connect gate="-A" pin="IOA4" pad="G18"/>
<connect gate="-A" pin="IOA5" pad="E2"/>
<connect gate="-A" pin="IOA6" pad="D2"/>
<connect gate="-A" pin="IOA7" pad="E3"/>
<connect gate="-A" pin="IOA8" pad="C1"/>
<connect gate="-A" pin="IOA9" pad="D1"/>
<connect gate="-B" pin="IOB1" pad="F21"/>
<connect gate="-B" pin="IOB10" pad="G19"/>
<connect gate="-B" pin="IOB12" pad="G20"/>
<connect gate="-B" pin="IOB13" pad="F2"/>
<connect gate="-B" pin="IOB16" pad="F22"/>
<connect gate="-B" pin="IOB2" pad="F16"/>
<connect gate="-B" pin="IOB3" pad="G17"/>
<connect gate="-B" pin="IOB4" pad="H7"/>
<connect gate="-B" pin="IOB5" pad="G5"/>
<connect gate="-B" pin="IOB6" pad="G4"/>
<connect gate="-B" pin="IOB7" pad="F3"/>
<connect gate="-B" pin="IOB8" pad="G6"/>
<connect gate="-B" pin="IOB9" pad="F4"/>
<connect gate="-C" pin="IOC1" pad="G22"/>
<connect gate="-C" pin="IOC10" pad="H3"/>
<connect gate="-C" pin="IOC11" pad="F15"/>
<connect gate="-C" pin="IOC12" pad="H6"/>
<connect gate="-C" pin="IOC13" pad="H18"/>
<connect gate="-C" pin="IOC15" pad="H17"/>
<connect gate="-C" pin="IOC16" pad="G16"/>
<connect gate="-C" pin="IOC2" pad="H21"/>
<connect gate="-C" pin="IOC3" pad="H1"/>
<connect gate="-C" pin="IOC4" pad="H4"/>
<connect gate="-C" pin="IOC5" pad="H5"/>
<connect gate="-C" pin="IOC6" pad="G2"/>
<connect gate="-C" pin="IOC8" pad="J7"/>
<connect gate="-C" pin="IOC9" pad="H19"/>
<connect gate="-D" pin="IOD1" pad="K17"/>
<connect gate="-D" pin="IOD10" pad="J3"/>
<connect gate="-D" pin="IOD12" pad="J5"/>
<connect gate="-D" pin="IOD13" pad="J2"/>
<connect gate="-D" pin="IOD14" pad="J21"/>
<connect gate="-D" pin="IOD15" pad="K7"/>
<connect gate="-D" pin="IOD16" pad="J18"/>
<connect gate="-D" pin="IOD2" pad="J19"/>
<connect gate="-D" pin="IOD3" pad="J22"/>
<connect gate="-D" pin="IOD4" pad="K19"/>
<connect gate="-D" pin="IOD5" pad="J1"/>
<connect gate="-D" pin="IOD6" pad="K8"/>
<connect gate="-D" pin="IOD7" pad="J6"/>
<connect gate="-D" pin="IOD8" pad="J4"/>
<connect gate="-D" pin="IOD9" pad="H22"/>
<connect gate="-E" pin="IOE1" pad="K21"/>
<connect gate="-E" pin="IOE11" pad="K18"/>
<connect gate="-E" pin="IOE12" pad="K2"/>
<connect gate="-E" pin="IOE13" pad="L7"/>
<connect gate="-E" pin="IOE14" pad="J17"/>
<connect gate="-E" pin="IOE16" pad="H16"/>
<connect gate="-E" pin="IOE2" pad="K22"/>
<connect gate="-E" pin="IOE3" pad="K1"/>
<connect gate="-E" pin="IOE4" pad="K4"/>
<connect gate="-E" pin="IOE5" pad="K6"/>
<connect gate="-E" pin="IOE6" pad="J16"/>
<connect gate="-E" pin="IOE8" pad="K5"/>
<connect gate="-E" pin="IOE9" pad="L8"/>
<connect gate="-F" pin="IOF1" pad="L21"/>
<connect gate="-F" pin="IOF11" pad="L19"/>
<connect gate="-F" pin="IOF12" pad="L17"/>
<connect gate="-F" pin="IOF13" pad="L5"/>
<connect gate="-F" pin="IOF14" pad="L6"/>
<connect gate="-F" pin="IOF15" pad="L3"/>
<connect gate="-F" pin="IOF16" pad="L2"/>
<connect gate="-F" pin="IOF2" pad="L18"/>
<connect gate="-F" pin="IOF3" pad="M8"/>
<connect gate="-F" pin="IOF4" pad="L1"/>
<connect gate="-F" pin="IOF5" pad="L4"/>
<connect gate="-F" pin="IOF6" pad="L20"/>
<connect gate="-F" pin="IOF7" pad="K16"/>
<connect gate="-F" pin="IOF8" pad="M7"/>
<connect gate="-F" pin="IOF9" pad="L22"/>
<connect gate="-G" pin="IOG1" pad="M18"/>
<connect gate="-G" pin="IOG10" pad="M22"/>
<connect gate="-G" pin="IOG11" pad="M21"/>
<connect gate="-G" pin="IOG12" pad="M19"/>
<connect gate="-G" pin="IOG13" pad="N8"/>
<connect gate="-G" pin="IOG15" pad="M17"/>
<connect gate="-G" pin="IOG16" pad="K15"/>
<connect gate="-G" pin="IOG2" pad="L16"/>
<connect gate="-G" pin="IOG3" pad="M2"/>
<connect gate="-G" pin="IOG4" pad="M3"/>
<connect gate="-G" pin="IOG5" pad="M4"/>
<connect gate="-G" pin="IOG6" pad="M1"/>
<connect gate="-G" pin="IOG8" pad="M6"/>
<connect gate="-G" pin="IOG9" pad="M5"/>
<connect gate="-H" pin="IOH1" pad="N22"/>
<connect gate="-H" pin="IOH10" pad="N1"/>
<connect gate="-H" pin="IOH11" pad="N6"/>
<connect gate="-H" pin="IOH12" pad="N21"/>
<connect gate="-H" pin="IOH13" pad="G14"/>
<connect gate="-H" pin="IOH14" pad="P7"/>
<connect gate="-H" pin="IOH15" pad="P22"/>
<connect gate="-H" pin="IOH16" pad="L15"/>
<connect gate="-H" pin="IOH2" pad="N19"/>
<connect gate="-H" pin="IOH3" pad="N18"/>
<connect gate="-H" pin="IOH4" pad="N5"/>
<connect gate="-H" pin="IOH5" pad="N7"/>
<connect gate="-H" pin="IOH7" pad="N4"/>
<connect gate="-H" pin="IOH8" pad="N2"/>
<connect gate="-I" pin="IOI1" pad="N17"/>
<connect gate="-I" pin="IOI10" pad="P21"/>
<connect gate="-I" pin="IOI11" pad="P20"/>
<connect gate="-I" pin="IOI12" pad="P18"/>
<connect gate="-I" pin="IOI13" pad="P6"/>
<connect gate="-I" pin="IOI14" pad="M16"/>
<connect gate="-I" pin="IOI15" pad="P19"/>
<connect gate="-I" pin="IOI16" pad="R21"/>
<connect gate="-I" pin="IOI2" pad="M15"/>
<connect gate="-I" pin="IOI3" pad="P5"/>
<connect gate="-I" pin="IOI4" pad="P2"/>
<connect gate="-I" pin="IOI5" pad="P3"/>
<connect gate="-I" pin="IOI6" pad="P1"/>
<connect gate="-I" pin="IOI7" pad="R7"/>
<connect gate="-I" pin="IOI9" pad="P4"/>
<connect gate="-J" pin="IOJ1" pad="R19"/>
<connect gate="-J" pin="IOJ10" pad="N15"/>
<connect gate="-J" pin="IOJ11" pad="T9"/>
<connect gate="-J" pin="IOJ12" pad="R5"/>
<connect gate="-J" pin="IOJ13" pad="N16"/>
<connect gate="-J" pin="IOJ14" pad="T2"/>
<connect gate="-J" pin="IOJ15" pad="R18"/>
<connect gate="-J" pin="IOJ16" pad="T21"/>
<connect gate="-J" pin="IOJ2" pad="P16"/>
<connect gate="-J" pin="IOJ3" pad="T8"/>
<connect gate="-J" pin="IOJ4" pad="R3"/>
<connect gate="-J" pin="IOJ5" pad="R4"/>
<connect gate="-J" pin="IOJ6" pad="R6"/>
<connect gate="-J" pin="IOJ7" pad="P17"/>
<connect gate="-J" pin="IOJ8" pad="R2"/>
<connect gate="-J" pin="IOJ9" pad="R20"/>
<connect gate="-K" pin="IOK1" pad="G13"/>
<connect gate="-K" pin="IOK10" pad="T5"/>
<connect gate="-K" pin="IOK11" pad="R17"/>
<connect gate="-K" pin="IOK13" pad="T20"/>
<connect gate="-K" pin="IOK14" pad="U5"/>
<connect gate="-K" pin="IOK15" pad="U21"/>
<connect gate="-K" pin="IOK2" pad="U20"/>
<connect gate="-K" pin="IOK3" pad="U2"/>
<connect gate="-K" pin="IOK4" pad="T6"/>
<connect gate="-K" pin="IOK5" pad="T4"/>
<connect gate="-K" pin="IOK6" pad="U22"/>
<connect gate="-K" pin="IOK7" pad="T19"/>
<connect gate="-K" pin="IOK8" pad="U6"/>
<connect gate="-K" pin="IOK9" pad="U1"/>
<connect gate="-L" pin="IOL1" pad="V21"/>
<connect gate="-L" pin="IOL10" pad="U19"/>
<connect gate="-L" pin="IOL11" pad="W2"/>
<connect gate="-L" pin="IOL12" pad="H13"/>
<connect gate="-L" pin="IOL13" pad="V2"/>
<connect gate="-L" pin="IOL14" pad="W22"/>
<connect gate="-L" pin="IOL15" pad="V20"/>
<connect gate="-L" pin="IOL16" pad="T18"/>
<connect gate="-L" pin="IOL2" pad="R16"/>
<connect gate="-L" pin="IOL3" pad="T17"/>
<connect gate="-L" pin="IOL4" pad="W1"/>
<connect gate="-L" pin="IOL5" pad="U3"/>
<connect gate="-L" pin="IOL6" pad="V6"/>
<connect gate="-L" pin="IOL8" pad="V1"/>
<connect gate="G1" pin="GND" pad="AA1"/>
<connect gate="G10" pin="GND" pad="B2"/>
<connect gate="G11" pin="GND" pad="B17"/>
<connect gate="G12" pin="GND" pad="B21"/>
<connect gate="G13" pin="GND" pad="B22"/>
<connect gate="G14" pin="GND" pad="C2"/>
<connect gate="G15" pin="GND" pad="C21"/>
<connect gate="G16" pin="GND" pad="E21"/>
<connect gate="G17" pin="GND" pad="G3"/>
<connect gate="G18" pin="GND" pad="G21"/>
<connect gate="G19" pin="GND" pad="H2"/>
<connect gate="G2" pin="GND" pad="AA6"/>
<connect gate="G20" pin="GND" pad="H8"/>
<connect gate="G21" pin="GND" pad="H15"/>
<connect gate="G22" pin="GND" pad="J9"/>
<connect gate="G23" pin="GND" pad="J14"/>
<connect gate="G24" pin="GND" pad="J20"/>
<connect gate="G25" pin="GND" pad="K3"/>
<connect gate="G26" pin="GND" pad="K10"/>
<connect gate="G27" pin="GND" pad="K12"/>
<connect gate="G28" pin="GND" pad="K13"/>
<connect gate="G29" pin="GND" pad="L11"/>
<connect gate="G3" pin="GND" pad="AA22"/>
<connect gate="G30" pin="GND" pad="L12"/>
<connect gate="G31" pin="GND" pad="M11"/>
<connect gate="G32" pin="GND" pad="M12"/>
<connect gate="G33" pin="GND" pad="M20"/>
<connect gate="G34" pin="GND" pad="N10"/>
<connect gate="G35" pin="GND" pad="N13"/>
<connect gate="G36" pin="GND" pad="P9"/>
<connect gate="G37" pin="GND" pad="P14"/>
<connect gate="G38" pin="GND" pad="R8"/>
<connect gate="G39" pin="GND" pad="R15"/>
<connect gate="G4" pin="GND" pad="AB11"/>
<connect gate="G40" pin="GND" pad="R22"/>
<connect gate="G41" pin="GND" pad="T1"/>
<connect gate="G42" pin="GND" pad="V3"/>
<connect gate="G43" pin="GND" pad="W11"/>
<connect gate="G44" pin="GND" pad="W20"/>
<connect gate="G45" pin="GND" pad="Y1"/>
<connect gate="G46" pin="GND" pad="Y2"/>
<connect gate="G47" pin="GND" pad="Y3"/>
<connect gate="G48" pin="GND" pad="Y21"/>
<connect gate="G49" pin="GND" pad="Y22"/>
<connect gate="G5" pin="GND" pad="AB16"/>
<connect gate="G6" pin="GND" pad="A1"/>
<connect gate="G7" pin="GND" pad="A8"/>
<connect gate="G8" pin="GND" pad="A22"/>
<connect gate="G9" pin="GND" pad="B1"/>
<connect gate="V1" pin="VCC" pad="AA12"/>
<connect gate="V10" pin="VCC" pad="L13"/>
<connect gate="V11" pin="VCC" pad="M10"/>
<connect gate="V12" pin="VCC" pad="M13"/>
<connect gate="V13" pin="VCC" pad="M14"/>
<connect gate="V14" pin="VCC" pad="N12"/>
<connect gate="V15" pin="VCC" pad="P8"/>
<connect gate="V16" pin="VCC" pad="P10"/>
<connect gate="V17" pin="VCC" pad="P12"/>
<connect gate="V18" pin="VCC" pad="P15"/>
<connect gate="V19" pin="VCC" pad="R14"/>
<connect gate="V2" pin="VCC" pad="C11"/>
<connect gate="V20" pin="VCC" pad="V5"/>
<connect gate="V21" pin="VCC" pad="W21"/>
<connect gate="V22" pin="VCC" pad="Y8"/>
<connect gate="V3" pin="VCC" pad="C15"/>
<connect gate="V4" pin="VCC" pad="H14"/>
<connect gate="V5" pin="VCC" pad="J8"/>
<connect gate="V6" pin="VCC" pad="J10"/>
<connect gate="V7" pin="VCC" pad="J12"/>
<connect gate="V8" pin="VCC" pad="J15"/>
<connect gate="V9" pin="VCC" pad="L9"/>
<connect gate="VO1" pin="VCCIO" pad="AB13"/>
<connect gate="VO10" pin="VCCIO" pad="J11"/>
<connect gate="VO11" pin="VCCIO" pad="J13"/>
<connect gate="VO12" pin="VCCIO" pad="K9"/>
<connect gate="VO13" pin="VCCIO" pad="K11"/>
<connect gate="VO14" pin="VCCIO" pad="K14"/>
<connect gate="VO15" pin="VCCIO" pad="K20"/>
<connect gate="VO16" pin="VCCIO" pad="L14"/>
<connect gate="VO17" pin="VCCIO" pad="M9"/>
<connect gate="VO18" pin="VCCIO" pad="N3"/>
<connect gate="VO19" pin="VCCIO" pad="N9"/>
<connect gate="VO2" pin="VCCIO" pad="A6"/>
<connect gate="VO20" pin="VCCIO" pad="N11"/>
<connect gate="VO21" pin="VCCIO" pad="N14"/>
<connect gate="VO22" pin="VCCIO" pad="N20"/>
<connect gate="VO23" pin="VCCIO" pad="P13"/>
<connect gate="VO24" pin="VCCIO" pad="R1"/>
<connect gate="VO25" pin="VCCIO" pad="R9"/>
<connect gate="VO26" pin="VCCIO" pad="T3"/>
<connect gate="VO27" pin="VCCIO" pad="T15"/>
<connect gate="VO28" pin="VCCIO" pad="T22"/>
<connect gate="VO29" pin="VCCIO" pad="V22"/>
<connect gate="VO3" pin="VCCIO" pad="A13"/>
<connect gate="VO4" pin="VCCIO" pad="B5"/>
<connect gate="VO5" pin="VCCIO" pad="E1"/>
<connect gate="VO6" pin="VCCIO" pad="G1"/>
<connect gate="VO7" pin="VCCIO" pad="G15"/>
<connect gate="VO8" pin="VCCIO" pad="H9"/>
<connect gate="VO9" pin="VCCIO" pad="H20"/>
<connect gate="_" pin="/CE" pad="E4"/>
<connect gate="_" pin="/CEO" pad="E19"/>
<connect gate="_" pin="/CONFIG" pad="T7"/>
<connect gate="_" pin="/STATUS" pad="W19"/>
<connect gate="_" pin="CONF_DONE" pad="F18"/>
<connect gate="_" pin="DATA0" pad="D4"/>
<connect gate="_" pin="DCLK" pad="E5"/>
<connect gate="_" pin="GCLK" pad="D12"/>
<connect gate="_" pin="GCLK1" pad="P11"/>
<connect gate="_" pin="IN0" pad="R12"/>
<connect gate="_" pin="IN1" pad="V11"/>
<connect gate="_" pin="IN2" pad="H11"/>
<connect gate="_" pin="IN3" pad="E12"/>
<connect gate="_" pin="MSEL0" pad="U4"/>
<connect gate="_" pin="MSEL1" pad="V4"/>
<connect gate="_" pin="TCK" pad="E18"/>
<connect gate="_" pin="TDI" pad="F5"/>
<connect gate="_" pin="TDO" pad="F19"/>
<connect gate="_" pin="TMS" pad="U18"/>
<connect gate="_" pin="TRST" pad="V19"/>
<connect gate="_" pin="VCC_CKLK" pad="L10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K100AFC484-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8791"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K130V-P240" prefix="IC">
<description>&lt;b&gt;EPF10K130&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="K_CTRL"/>
<gate name="-AB" symbol="AB6"/>
<gate name="-CD" symbol="CD6"/>
<gate name="-EF" symbol="EF6"/>
<gate name="-GH" symbol="GH6"/>
<gate name="-IJ" symbol="IJ4"/>
<gate name="-KL" symbol="KL4"/>
<gate name="-MN" symbol="MN4"/>
<gate name="-OP" symbol="OP5"/>
<gate name="-1" symbol="122-240"/>
<gate name="-2" symbol="192-240"/>
<gate name="-3" symbol="261-240"/>
<gate name="-4" symbol="322-240"/>
<gate name="-5" symbol="403-240"/>
<gate name="-6" symbol="511-240"/>
<gate name="-7" symbol="522-240"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="19" symbol="VCCIO"/>
<gate name="20" symbol="VCCIO"/>
<gate name="21" symbol="VCCIO"/>
<gate name="22" symbol="VCCIO"/>
<gate name="23" symbol="GND"/>
<gate name="24" symbol="GND"/>
<gate name="25" symbol="GND"/>
<gate name="26" symbol="GND"/>
<gate name="27" symbol="GND"/>
<gate name="28" symbol="GND"/>
<gate name="29" symbol="GND"/>
<gate name="30" symbol="GND"/>
<gate name="31" symbol="GND"/>
<gate name="32" symbol="GND"/>
<gate name="33" symbol="GND"/>
<gate name="34" symbol="GND"/>
<gate name="35" symbol="GND"/>
<gate name="36" symbol="GND"/>
<gate name="37" symbol="GND"/>
<gate name="38" symbol="GND"/>
<gate name="39" symbol="GND"/>
<gate name="40" symbol="GND"/>
</gates>
<devices>
<device name="" package="PQFP240">
<connects>
<connect gate="-1" pin="IO101" pad="110"/>
<connect gate="-1" pin="IO102" pad="182"/>
<connect gate="-1" pin="IO11" pad="120"/>
<connect gate="-1" pin="IO111" pad="109"/>
<connect gate="-1" pin="IO112" pad="183"/>
<connect gate="-1" pin="IO121" pad="108"/>
<connect gate="-1" pin="IO122" pad="184"/>
<connect gate="-1" pin="IO21" pad="119"/>
<connect gate="-1" pin="IO31" pad="118"/>
<connect gate="-1" pin="IO41" pad="117"/>
<connect gate="-1" pin="IO51" pad="116"/>
<connect gate="-1" pin="IO61" pad="115"/>
<connect gate="-1" pin="IO71" pad="114"/>
<connect gate="-1" pin="IO81" pad="113"/>
<connect gate="-1" pin="IO91" pad="111"/>
<connect gate="-1" pin="IO92" pad="181"/>
<connect gate="-2" pin="IO123" pad="185"/>
<connect gate="-2" pin="IO131" pad="107"/>
<connect gate="-2" pin="IO132" pad="186"/>
<connect gate="-2" pin="IO141" pad="106"/>
<connect gate="-2" pin="IO142" pad="187"/>
<connect gate="-2" pin="IO143" pad="188"/>
<connect gate="-2" pin="IO151" pad="105"/>
<connect gate="-2" pin="IO152" pad="190"/>
<connect gate="-2" pin="IO161" pad="103"/>
<connect gate="-2" pin="IO162" pad="191"/>
<connect gate="-2" pin="IO163" pad="192"/>
<connect gate="-2" pin="IO171" pad="193"/>
<connect gate="-2" pin="IO181" pad="102"/>
<connect gate="-2" pin="IO182" pad="194"/>
<connect gate="-2" pin="IO191" pad="101"/>
<connect gate="-2" pin="IO192" pad="195"/>
<connect gate="-3" pin="IO193" pad="196"/>
<connect gate="-3" pin="IO201" pad="100"/>
<connect gate="-3" pin="IO202" pad="198"/>
<connect gate="-3" pin="IO211" pad="99"/>
<connect gate="-3" pin="IO212" pad="199"/>
<connect gate="-3" pin="IO221" pad="200"/>
<connect gate="-3" pin="IO222" pad="201"/>
<connect gate="-3" pin="IO231" pad="98"/>
<connect gate="-3" pin="IO232" pad="202"/>
<connect gate="-3" pin="IO233" pad="203"/>
<connect gate="-3" pin="IO241" pad="97"/>
<connect gate="-3" pin="IO242" pad="204"/>
<connect gate="-3" pin="IO251" pad="95"/>
<connect gate="-3" pin="IO252" pad="206"/>
<connect gate="-3" pin="IO253" pad="207"/>
<connect gate="-3" pin="IO261" pad="94"/>
<connect gate="-4" pin="IO262" pad="208"/>
<connect gate="-4" pin="IO263" pad="209"/>
<connect gate="-4" pin="IO271" pad="87"/>
<connect gate="-4" pin="IO272" pad="88"/>
<connect gate="-4" pin="IO273" pad="213"/>
<connect gate="-4" pin="IO281" pad="86"/>
<connect gate="-4" pin="IO282" pad="214"/>
<connect gate="-4" pin="IO283" pad="215"/>
<connect gate="-4" pin="IO291" pad="83"/>
<connect gate="-4" pin="IO292" pad="84"/>
<connect gate="-4" pin="IO293" pad="217"/>
<connect gate="-4" pin="IO301" pad="82"/>
<connect gate="-4" pin="IO302" pad="218"/>
<connect gate="-4" pin="IO311" pad="81"/>
<connect gate="-4" pin="IO321" pad="80"/>
<connect gate="-4" pin="IO322" pad="219"/>
<connect gate="-5" pin="IO331" pad="78"/>
<connect gate="-5" pin="IO332" pad="79"/>
<connect gate="-5" pin="IO333" pad="220"/>
<connect gate="-5" pin="IO341" pad="75"/>
<connect gate="-5" pin="IO351" pad="74"/>
<connect gate="-5" pin="IO352" pad="221"/>
<connect gate="-5" pin="IO361" pad="73"/>
<connect gate="-5" pin="IO362" pad="222"/>
<connect gate="-5" pin="IO363" pad="223"/>
<connect gate="-5" pin="IO371" pad="225"/>
<connect gate="-5" pin="IO381" pad="72"/>
<connect gate="-5" pin="IO382" pad="226"/>
<connect gate="-5" pin="IO391" pad="227"/>
<connect gate="-5" pin="IO401" pad="70"/>
<connect gate="-5" pin="IO402" pad="71"/>
<connect gate="-5" pin="IO403" pad="228"/>
<connect gate="-6" pin="IO411" pad="229"/>
<connect gate="-6" pin="IO421" pad="68"/>
<connect gate="-6" pin="IO431" pad="67"/>
<connect gate="-6" pin="IO432" pad="230"/>
<connect gate="-6" pin="IO441" pad="231"/>
<connect gate="-6" pin="IO451" pad="66"/>
<connect gate="-6" pin="IO452" pad="233"/>
<connect gate="-6" pin="IO461" pad="65"/>
<connect gate="-6" pin="IO462" pad="234"/>
<connect gate="-6" pin="IO471" pad="235"/>
<connect gate="-6" pin="IO481" pad="64"/>
<connect gate="-6" pin="IO491" pad="63"/>
<connect gate="-6" pin="IO492" pad="236"/>
<connect gate="-6" pin="IO501" pad="237"/>
<connect gate="-6" pin="IO502" pad="238"/>
<connect gate="-6" pin="IO511" pad="62"/>
<connect gate="-7" pin="IO512" pad="239"/>
<connect gate="-7" pin="IO521" pad="61"/>
<connect gate="-7" pin="IO522" pad="240"/>
<connect gate="-AB" pin="IOA1" pad="6"/>
<connect gate="-AB" pin="IOA2" pad="7"/>
<connect gate="-AB" pin="IOA3" pad="8"/>
<connect gate="-AB" pin="IOA4" pad="9"/>
<connect gate="-AB" pin="IOA5" pad="11"/>
<connect gate="-AB" pin="IOA6" pad="175"/>
<connect gate="-AB" pin="IOB1" pad="12"/>
<connect gate="-AB" pin="IOB2" pad="13"/>
<connect gate="-AB" pin="IOB3" pad="14"/>
<connect gate="-AB" pin="IOB4" pad="15"/>
<connect gate="-AB" pin="IOB5" pad="173"/>
<connect gate="-AB" pin="IOB6" pad="174"/>
<connect gate="-CD" pin="IOC1" pad="17"/>
<connect gate="-CD" pin="IOC2" pad="18"/>
<connect gate="-CD" pin="IOC3" pad="19"/>
<connect gate="-CD" pin="IOC4" pad="169"/>
<connect gate="-CD" pin="IOC5" pad="171"/>
<connect gate="-CD" pin="IOC6" pad="172"/>
<connect gate="-CD" pin="IOD1" pad="21"/>
<connect gate="-CD" pin="IOD2" pad="23"/>
<connect gate="-CD" pin="IOD3" pad="24"/>
<connect gate="-CD" pin="IOD4" pad="25"/>
<connect gate="-CD" pin="IOD5" pad="26"/>
<connect gate="-CD" pin="IOD6" pad="168"/>
<connect gate="-EF" pin="IOE1" pad="28"/>
<connect gate="-EF" pin="IOE2" pad="162"/>
<connect gate="-EF" pin="IOE3" pad="163"/>
<connect gate="-EF" pin="IOE4" pad="164"/>
<connect gate="-EF" pin="IOE5" pad="166"/>
<connect gate="-EF" pin="IOE6" pad="167"/>
<connect gate="-EF" pin="IOF1" pad="29"/>
<connect gate="-EF" pin="IOF2" pad="30"/>
<connect gate="-EF" pin="IOF3" pad="156"/>
<connect gate="-EF" pin="IOF4" pad="157"/>
<connect gate="-EF" pin="IOF5" pad="158"/>
<connect gate="-EF" pin="IOF6" pad="161"/>
<connect gate="-GH" pin="IOG1" pad="31"/>
<connect gate="-GH" pin="IOG2" pad="33"/>
<connect gate="-GH" pin="IOG3" pad="34"/>
<connect gate="-GH" pin="IOG4" pad="152"/>
<connect gate="-GH" pin="IOG5" pad="153"/>
<connect gate="-GH" pin="IOG6" pad="154"/>
<connect gate="-GH" pin="IOH1" pad="35"/>
<connect gate="-GH" pin="IOH2" pad="36"/>
<connect gate="-GH" pin="IOH3" pad="38"/>
<connect gate="-GH" pin="IOH4" pad="149"/>
<connect gate="-GH" pin="IOH5" pad="151"/>
<connect gate="-IJ" pin="IOI1" pad="39"/>
<connect gate="-IJ" pin="IOI2" pad="40"/>
<connect gate="-IJ" pin="IOI3" pad="146"/>
<connect gate="-IJ" pin="IOI4" pad="147"/>
<connect gate="-IJ" pin="IOI5" pad="148"/>
<connect gate="-IJ" pin="IOJ1" pad="41"/>
<connect gate="-IJ" pin="IOJ2" pad="43"/>
<connect gate="-IJ" pin="IOJ3" pad="143"/>
<connect gate="-IJ" pin="IOJ4" pad="144"/>
<connect gate="-KL" pin="IOK1" pad="44"/>
<connect gate="-KL" pin="IOK2" pad="45"/>
<connect gate="-KL" pin="IOK3" pad="141"/>
<connect gate="-KL" pin="IOK4" pad="142"/>
<connect gate="-KL" pin="IOL1" pad="46"/>
<connect gate="-KL" pin="IOL2" pad="137"/>
<connect gate="-KL" pin="IOL3" pad="138"/>
<connect gate="-KL" pin="IOL4" pad="139"/>
<connect gate="-MN" pin="IOM1" pad="48"/>
<connect gate="-MN" pin="IOM2" pad="49"/>
<connect gate="-MN" pin="IOM3" pad="134"/>
<connect gate="-MN" pin="IOM4" pad="136"/>
<connect gate="-MN" pin="ION1" pad="50"/>
<connect gate="-MN" pin="ION2" pad="51"/>
<connect gate="-MN" pin="ION3" pad="132"/>
<connect gate="-MN" pin="ION4" pad="133"/>
<connect gate="-OP" pin="IOO1" pad="53"/>
<connect gate="-OP" pin="IOO2" pad="54"/>
<connect gate="-OP" pin="IOO3" pad="129"/>
<connect gate="-OP" pin="IOO4" pad="131"/>
<connect gate="-OP" pin="IOP1" pad="55"/>
<connect gate="-OP" pin="IOP2" pad="56"/>
<connect gate="-OP" pin="IOP3" pad="126"/>
<connect gate="-OP" pin="IOP4" pad="127"/>
<connect gate="-OP" pin="IOP5" pad="128"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="10" pin="VCC" pad="150"/>
<connect gate="11" pin="VCC" pad="159"/>
<connect gate="12" pin="VCC" pad="170"/>
<connect gate="13" pin="VCCIO" pad="16"/>
<connect gate="14" pin="VCCIO" pad="37"/>
<connect gate="15" pin="VCCIO" pad="57"/>
<connect gate="16" pin="VCCIO" pad="77"/>
<connect gate="17" pin="VCCIO" pad="112"/>
<connect gate="18" pin="VCCIO" pad="140"/>
<connect gate="19" pin="VCCIO" pad="160"/>
<connect gate="2" pin="VCC" pad="20"/>
<connect gate="20" pin="VCCIO" pad="189"/>
<connect gate="21" pin="VCCIO" pad="205"/>
<connect gate="22" pin="VCCIO" pad="224"/>
<connect gate="23" pin="GND" pad="10"/>
<connect gate="24" pin="GND" pad="22"/>
<connect gate="25" pin="GND" pad="32"/>
<connect gate="26" pin="GND" pad="42"/>
<connect gate="27" pin="GND" pad="52"/>
<connect gate="28" pin="GND" pad="69"/>
<connect gate="29" pin="GND" pad="85"/>
<connect gate="3" pin="VCC" pad="27"/>
<connect gate="30" pin="GND" pad="93"/>
<connect gate="31" pin="GND" pad="104"/>
<connect gate="32" pin="GND" pad="125"/>
<connect gate="33" pin="GND" pad="135"/>
<connect gate="34" pin="GND" pad="145"/>
<connect gate="35" pin="GND" pad="155"/>
<connect gate="36" pin="GND" pad="165"/>
<connect gate="37" pin="GND" pad="176"/>
<connect gate="38" pin="GND" pad="197"/>
<connect gate="39" pin="GND" pad="216"/>
<connect gate="4" pin="VCC" pad="47"/>
<connect gate="40" pin="GND" pad="232"/>
<connect gate="5" pin="VCC" pad="76"/>
<connect gate="6" pin="VCC" pad="89"/>
<connect gate="7" pin="VCC" pad="96"/>
<connect gate="8" pin="VCC" pad="122"/>
<connect gate="9" pin="VCC" pad="130"/>
<connect gate="_" pin="/CE" pad="178"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="121"/>
<connect gate="_" pin="/STATUS" pad="60"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="180"/>
<connect gate="_" pin="DCLK" pad="179"/>
<connect gate="_" pin="GCLK0" pad="91"/>
<connect gate="_" pin="GCLK1" pad="211"/>
<connect gate="_" pin="IN0" pad="90"/>
<connect gate="_" pin="IN1" pad="92"/>
<connect gate="_" pin="IN2" pad="210"/>
<connect gate="_" pin="IN3" pad="212"/>
<connect gate="_" pin="MSEL0" pad="124"/>
<connect gate="_" pin="MSEL1" pad="123"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="177"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="58"/>
<connect gate="_" pin="TRST" pad="59"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K100-FBGA256" prefix="IC">
<description>&lt;b&gt;EPF10K100&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100F256C"/>
<gate name="-1" symbol="122-256"/>
<gate name="-2" symbol="192-256"/>
<gate name="-3" symbol="261-256"/>
<gate name="-4" symbol="323-256"/>
<gate name="-5" symbol="411-256"/>
<gate name="-6" symbol="504-256"/>
<gate name="-7" symbol="522-256"/>
<gate name="-AB" symbol="AB-256"/>
<gate name="-CD" symbol="CD-256"/>
<gate name="-EF" symbol="EF-256"/>
<gate name="-GH" symbol="GH-256"/>
<gate name="-IJ" symbol="IJ-256"/>
<gate name="-KL" symbol="KL-256"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="FBGA256">
<connects>
<connect gate="-1" pin="IO101" pad="A2"/>
<connect gate="-1" pin="IO11" pad="T1"/>
<connect gate="-1" pin="IO111" pad="C3"/>
<connect gate="-1" pin="IO113" pad="R5"/>
<connect gate="-1" pin="IO121" pad="A3"/>
<connect gate="-1" pin="IO122" pad="B4"/>
<connect gate="-1" pin="IO21" pad="T2"/>
<connect gate="-1" pin="IO31" pad="T3"/>
<connect gate="-1" pin="IO32" pad="R3"/>
<connect gate="-1" pin="IO41" pad="P3"/>
<connect gate="-1" pin="IO51" pad="P4"/>
<connect gate="-1" pin="IO61" pad="R4"/>
<connect gate="-1" pin="IO71" pad="T4"/>
<connect gate="-1" pin="IO81" pad="N5"/>
<connect gate="-1" pin="IO91" pad="P5"/>
<connect gate="-1" pin="IO92" pad="B3"/>
<connect gate="-2" pin="IO124" pad="T5"/>
<connect gate="-2" pin="IO131" pad="N6"/>
<connect gate="-2" pin="IO132" pad="A4"/>
<connect gate="-2" pin="IO141" pad="P6"/>
<connect gate="-2" pin="IO142" pad="C4"/>
<connect gate="-2" pin="IO143" pad="D4"/>
<connect gate="-2" pin="IO151" pad="R6"/>
<connect gate="-2" pin="IO152" pad="B5"/>
<connect gate="-2" pin="IO161" pad="T6"/>
<connect gate="-2" pin="IO162" pad="C5"/>
<connect gate="-2" pin="IO164" pad="A5"/>
<connect gate="-2" pin="IO171" pad="D5"/>
<connect gate="-2" pin="IO181" pad="M7"/>
<connect gate="-2" pin="IO182" pad="E4"/>
<connect gate="-2" pin="IO191" pad="N7"/>
<connect gate="-2" pin="IO192" pad="A6"/>
<connect gate="-3" pin="IO194" pad="B6"/>
<connect gate="-3" pin="IO201" pad="C6"/>
<connect gate="-3" pin="IO202" pad="P7"/>
<connect gate="-3" pin="IO211" pad="R7"/>
<connect gate="-3" pin="IO212" pad="D6"/>
<connect gate="-3" pin="IO221" pad="A7"/>
<connect gate="-3" pin="IO222" pad="B7"/>
<connect gate="-3" pin="IO231" pad="T7"/>
<connect gate="-3" pin="IO232" pad="D7"/>
<connect gate="-3" pin="IO234" pad="C7"/>
<connect gate="-3" pin="IO241" pad="M8"/>
<connect gate="-3" pin="IO242" pad="E7"/>
<connect gate="-3" pin="IO251" pad="N8"/>
<connect gate="-3" pin="IO252" pad="A8"/>
<connect gate="-3" pin="IO253" pad="B8"/>
<connect gate="-3" pin="IO261" pad="D8"/>
<connect gate="-4" pin="IO263" pad="C8"/>
<connect gate="-4" pin="IO264" pad="P8"/>
<connect gate="-4" pin="IO271" pad="R9"/>
<connect gate="-4" pin="IO272" pad="C9"/>
<connect gate="-4" pin="IO273" pad="T9"/>
<connect gate="-4" pin="IO281" pad="P9"/>
<connect gate="-4" pin="IO282" pad="D9"/>
<connect gate="-4" pin="IO284" pad="E9"/>
<connect gate="-4" pin="IO291" pad="R10"/>
<connect gate="-4" pin="IO293" pad="N9"/>
<connect gate="-4" pin="IO294" pad="A10"/>
<connect gate="-4" pin="IO301" pad="T10"/>
<connect gate="-4" pin="IO302" pad="B10"/>
<connect gate="-4" pin="IO311" pad="P10"/>
<connect gate="-4" pin="IO321" pad="N10"/>
<connect gate="-4" pin="IO323" pad="C10"/>
<connect gate="-5" pin="IO331" pad="N11"/>
<connect gate="-5" pin="IO332" pad="M10"/>
<connect gate="-5" pin="IO333" pad="D10"/>
<connect gate="-5" pin="IO341" pad="P11"/>
<connect gate="-5" pin="IO351" pad="T11"/>
<connect gate="-5" pin="IO352" pad="R11"/>
<connect gate="-5" pin="IO353" pad="E10"/>
<connect gate="-5" pin="IO361" pad="P12"/>
<connect gate="-5" pin="IO364" pad="A11"/>
<connect gate="-5" pin="IO371" pad="B11"/>
<connect gate="-5" pin="IO372" pad="R12"/>
<connect gate="-5" pin="IO381" pad="C11"/>
<connect gate="-5" pin="IO391" pad="D11"/>
<connect gate="-5" pin="IO402" pad="T12"/>
<connect gate="-5" pin="IO404" pad="A12"/>
<connect gate="-5" pin="IO411" pad="B12"/>
<connect gate="-6" pin="IO421" pad="N13"/>
<connect gate="-6" pin="IO431" pad="P13"/>
<connect gate="-6" pin="IO432" pad="C12"/>
<connect gate="-6" pin="IO441" pad="C13"/>
<connect gate="-6" pin="IO451" pad="T13"/>
<connect gate="-6" pin="IO452" pad="A13"/>
<connect gate="-6" pin="IO461" pad="B13"/>
<connect gate="-6" pin="IO462" pad="R13"/>
<connect gate="-6" pin="IO471" pad="D13"/>
<connect gate="-6" pin="IO481" pad="M13"/>
<connect gate="-6" pin="IO482" pad="D14"/>
<connect gate="-6" pin="IO491" pad="C14"/>
<connect gate="-6" pin="IO492" pad="T14"/>
<connect gate="-6" pin="IO501" pad="A14"/>
<connect gate="-6" pin="IO502" pad="B14"/>
<connect gate="-6" pin="IO504" pad="T15"/>
<connect gate="-7" pin="IO511" pad="R14"/>
<connect gate="-7" pin="IO512" pad="A15"/>
<connect gate="-7" pin="IO521" pad="R15"/>
<connect gate="-7" pin="IO522" pad="A16"/>
<connect gate="-AB" pin="IOA1" pad="E13"/>
<connect gate="-AB" pin="IOA2" pad="E14"/>
<connect gate="-AB" pin="IOA3" pad="D16"/>
<connect gate="-AB" pin="IOA4" pad="D15"/>
<connect gate="-AB" pin="IOA5" pad="D1"/>
<connect gate="-AB" pin="IOA6" pad="E3"/>
<connect gate="-AB" pin="IOA7" pad="D3"/>
<connect gate="-AB" pin="IOA8" pad="C1"/>
<connect gate="-AB" pin="IOA9" pad="D2"/>
<connect gate="-AB" pin="IOB1" pad="F13"/>
<connect gate="-AB" pin="IOB16" pad="E16"/>
<connect gate="-AB" pin="IOB2" pad="E15"/>
<connect gate="-AB" pin="IOB3" pad="F14"/>
<connect gate="-AB" pin="IOB5" pad="G5"/>
<connect gate="-AB" pin="IOB6" pad="E2"/>
<connect gate="-AB" pin="IOB7" pad="F4"/>
<connect gate="-AB" pin="IOB8" pad="F3"/>
<connect gate="-AB" pin="IOB9" pad="F1"/>
<connect gate="-CD" pin="IOC1" pad="G13"/>
<connect gate="-CD" pin="IOC11" pad="G12"/>
<connect gate="-CD" pin="IOC16" pad="F15"/>
<connect gate="-CD" pin="IOC2" pad="F16"/>
<connect gate="-CD" pin="IOC3" pad="G3"/>
<connect gate="-CD" pin="IOC4" pad="G4"/>
<connect gate="-CD" pin="IOC5" pad="E1"/>
<connect gate="-CD" pin="IOC6" pad="F2"/>
<connect gate="-CD" pin="IOD1" pad="G14"/>
<connect gate="-CD" pin="IOD2" pad="H12"/>
<connect gate="-CD" pin="IOD3" pad="G15"/>
<connect gate="-CD" pin="IOD4" pad="G16"/>
<connect gate="-CD" pin="IOD5" pad="G1"/>
<connect gate="-CD" pin="IOD6" pad="G2"/>
<connect gate="-CD" pin="IOD7" pad="H5"/>
<connect gate="-EF" pin="IOE1" pad="H13"/>
<connect gate="-EF" pin="IOE13" pad="H1"/>
<connect gate="-EF" pin="IOE2" pad="H14"/>
<connect gate="-EF" pin="IOE3" pad="H2"/>
<connect gate="-EF" pin="IOE4" pad="H3"/>
<connect gate="-EF" pin="IOE5" pad="H4"/>
<connect gate="-EF" pin="IOE6" pad="H16"/>
<connect gate="-EF" pin="IOF1" pad="J12"/>
<connect gate="-EF" pin="IOF14" pad="J5"/>
<connect gate="-EF" pin="IOF2" pad="J13"/>
<connect gate="-EF" pin="IOF3" pad="J1"/>
<connect gate="-EF" pin="IOF4" pad="J3"/>
<connect gate="-EF" pin="IOF5" pad="J4"/>
<connect gate="-EF" pin="IOF7" pad="H15"/>
<connect gate="-GH" pin="IOG1" pad="J16"/>
<connect gate="-GH" pin="IOG11" pad="J14"/>
<connect gate="-GH" pin="IOG2" pad="J15"/>
<connect gate="-GH" pin="IOG3" pad="K3"/>
<connect gate="-GH" pin="IOG4" pad="J2"/>
<connect gate="-GH" pin="IOG6" pad="K4"/>
<connect gate="-GH" pin="IOG8" pad="K1"/>
<connect gate="-GH" pin="IOH1" pad="K12"/>
<connect gate="-GH" pin="IOH2" pad="K16"/>
<connect gate="-GH" pin="IOH3" pad="K15"/>
<connect gate="-GH" pin="IOH4" pad="L3"/>
<connect gate="-GH" pin="IOH5" pad="K2"/>
<connect gate="-GH" pin="IOH8" pad="K5"/>
<connect gate="-IJ" pin="IOI1" pad="K14"/>
<connect gate="-IJ" pin="IOI12" pad="L16"/>
<connect gate="-IJ" pin="IOI14" pad="K13"/>
<connect gate="-IJ" pin="IOI2" pad="L14"/>
<connect gate="-IJ" pin="IOI3" pad="L2"/>
<connect gate="-IJ" pin="IOI5" pad="L1"/>
<connect gate="-IJ" pin="IOJ1" pad="L13"/>
<connect gate="-IJ" pin="IOJ10" pad="M14"/>
<connect gate="-IJ" pin="IOJ14" pad="L15"/>
<connect gate="-IJ" pin="IOJ15" pad="M2"/>
<connect gate="-IJ" pin="IOJ2" pad="M16"/>
<connect gate="-IJ" pin="IOJ3" pad="L4"/>
<connect gate="-KL" pin="IOK1" pad="N14"/>
<connect gate="-KL" pin="IOK11" pad="M15"/>
<connect gate="-KL" pin="IOK14" pad="M4"/>
<connect gate="-KL" pin="IOK2" pad="N16"/>
<connect gate="-KL" pin="IOK3" pad="M3"/>
<connect gate="-KL" pin="IOK4" pad="M1"/>
<connect gate="-KL" pin="IOL1" pad="N15"/>
<connect gate="-KL" pin="IOL11" pad="P2"/>
<connect gate="-KL" pin="IOL2" pad="P14"/>
<connect gate="-KL" pin="IOL3" pad="P16"/>
<connect gate="-KL" pin="IOL4" pad="N3"/>
<connect gate="-KL" pin="IOL5" pad="N1"/>
<connect gate="-KL" pin="IOL7" pad="N2"/>
<connect gate="G1" pin="GND" pad="E5"/>
<connect gate="G10" pin="GND" pad="J8"/>
<connect gate="G11" pin="GND" pad="J9"/>
<connect gate="G12" pin="GND" pad="K7"/>
<connect gate="G13" pin="GND" pad="K10"/>
<connect gate="G14" pin="GND" pad="L6"/>
<connect gate="G15" pin="GND" pad="L11"/>
<connect gate="G16" pin="GND" pad="M5"/>
<connect gate="G17" pin="GND" pad="M12"/>
<connect gate="G18" pin="GND" pad="T8"/>
<connect gate="G2" pin="GND" pad="E12"/>
<connect gate="G3" pin="GND" pad="F6"/>
<connect gate="G4" pin="GND" pad="F11"/>
<connect gate="G5" pin="GND" pad="G7"/>
<connect gate="G6" pin="GND" pad="G9"/>
<connect gate="G7" pin="GND" pad="G10"/>
<connect gate="G8" pin="GND" pad="H8"/>
<connect gate="G9" pin="GND" pad="H9"/>
<connect gate="V1" pin="VCC" pad="E11"/>
<connect gate="V10" pin="VCC" pad="J11"/>
<connect gate="V11" pin="VCC" pad="K9"/>
<connect gate="V12" pin="VCC" pad="L5"/>
<connect gate="V13" pin="VCC" pad="L7"/>
<connect gate="V14" pin="VCC" pad="L9"/>
<connect gate="V15" pin="VCC" pad="L12"/>
<connect gate="V16" pin="VCC" pad="M11"/>
<connect gate="V17" pin="VCC" pad="R2"/>
<connect gate="V2" pin="VCC" pad="F5"/>
<connect gate="V3" pin="VCC" pad="F7"/>
<connect gate="V4" pin="VCC" pad="F9"/>
<connect gate="V5" pin="VCC" pad="F12"/>
<connect gate="V6" pin="VCC" pad="H6"/>
<connect gate="V7" pin="VCC" pad="H7"/>
<connect gate="V8" pin="VCC" pad="H10"/>
<connect gate="V9" pin="VCC" pad="J7"/>
<connect gate="VO1" pin="VCCIO" pad="D12"/>
<connect gate="VO10" pin="VCCIO" pad="K6"/>
<connect gate="VO11" pin="VCCIO" pad="K8"/>
<connect gate="VO12" pin="VCCIO" pad="K11"/>
<connect gate="VO13" pin="VCCIO" pad="L10"/>
<connect gate="VO14" pin="VCCIO" pad="M6"/>
<connect gate="VO15" pin="VCCIO" pad="N12"/>
<connect gate="VO2" pin="VCCIO" pad="E6"/>
<connect gate="VO3" pin="VCCIO" pad="F8"/>
<connect gate="VO4" pin="VCCIO" pad="F10"/>
<connect gate="VO5" pin="VCCIO" pad="G6"/>
<connect gate="VO6" pin="VCCIO" pad="G8"/>
<connect gate="VO7" pin="VCCIO" pad="G11"/>
<connect gate="VO8" pin="VCCIO" pad="H11"/>
<connect gate="VO9" pin="VCCIO" pad="J6"/>
<connect gate="_" pin="/CE" pad="B1"/>
<connect gate="_" pin="/CEO" pad="B16"/>
<connect gate="_" pin="/CONFIG" pad="N4"/>
<connect gate="_" pin="/STATUS" pad="T16"/>
<connect gate="_" pin="CONF_DONE" pad="C15"/>
<connect gate="_" pin="DATA0" pad="A1"/>
<connect gate="_" pin="DCLK" pad="B2"/>
<connect gate="_" pin="GCLK" pad="A9"/>
<connect gate="_" pin="GCLK1" pad="L8"/>
<connect gate="_" pin="IN0" pad="M9"/>
<connect gate="_" pin="IN1" pad="R8"/>
<connect gate="_" pin="IN2" pad="E8"/>
<connect gate="_" pin="IN3" pad="B9"/>
<connect gate="_" pin="MSEL0" pad="P1"/>
<connect gate="_" pin="MSEL1" pad="R1"/>
<connect gate="_" pin="TCK" pad="B15"/>
<connect gate="_" pin="TDI" pad="C2"/>
<connect gate="_" pin="TDO" pad="C16"/>
<connect gate="_" pin="TMS" pad="P15"/>
<connect gate="_" pin="TRST" pad="R16"/>
<connect gate="_" pin="VCC_CKLK" pad="J10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K100EFC256-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8810"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K200-BGA672" prefix="IC">
<description>&lt;b&gt;EPF10K200&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="K200-CTR"/>
<gate name="-A" symbol="A11-672"/>
<gate name="-B" symbol="B11-672"/>
<gate name="-C" symbol="C10-672"/>
<gate name="-D" symbol="D11-672"/>
<gate name="-E" symbol="E11-672"/>
<gate name="-F" symbol="F10-672"/>
<gate name="-G" symbol="G11-672"/>
<gate name="-H" symbol="H11-672"/>
<gate name="-I" symbol="I11-672"/>
<gate name="-J" symbol="J13-672"/>
<gate name="-K" symbol="K11-672"/>
<gate name="-L" symbol="L10-672"/>
<gate name="-M" symbol="M11-672"/>
<gate name="-N" symbol="N11-672"/>
<gate name="-O" symbol="O10-672"/>
<gate name="-P" symbol="P11-672"/>
<gate name="-Q" symbol="Q11-672"/>
<gate name="-R" symbol="R10-672"/>
<gate name="-S" symbol="S11-672"/>
<gate name="-T" symbol="T11-672"/>
<gate name="-U" symbol="U10-672"/>
<gate name="-V" symbol="V11-672"/>
<gate name="-W" symbol="W11-672"/>
<gate name="-X" symbol="X10-672"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="-10" symbol="IO404"/>
<gate name="-11" symbol="IO444"/>
<gate name="-12" symbol="IO484"/>
<gate name="-13" symbol="IO524"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="G50" symbol="GND"/>
<gate name="G51" symbol="GND"/>
<gate name="G52" symbol="GND"/>
<gate name="G53" symbol="GND"/>
<gate name="G54" symbol="GND"/>
<gate name="G55" symbol="GND"/>
<gate name="G56" symbol="GND"/>
<gate name="G57" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC40" symbol="NC"/>
<gate name="NC41" symbol="NC"/>
<gate name="NC42" symbol="NC"/>
<gate name="NC43" symbol="NC"/>
<gate name="NC44" symbol="NC"/>
<gate name="NC45" symbol="NC"/>
<gate name="NC46" symbol="NC"/>
<gate name="NC47" symbol="NC"/>
<gate name="NC48" symbol="NC"/>
<gate name="NC49" symbol="NC"/>
<gate name="NC50" symbol="NC"/>
<gate name="NC51" symbol="NC"/>
<gate name="NC52" symbol="NC"/>
<gate name="NC53" symbol="NC"/>
<gate name="NC54" symbol="NC"/>
<gate name="NC55" symbol="NC"/>
<gate name="NC56" symbol="NC"/>
<gate name="NC57" symbol="NC"/>
<gate name="NC58" symbol="NC"/>
<gate name="NC59" symbol="NC"/>
<gate name="NC60" symbol="NC"/>
<gate name="NC61" symbol="NC"/>
<gate name="NC62" symbol="NC"/>
<gate name="NC63" symbol="NC"/>
<gate name="NC64" symbol="NC"/>
<gate name="NC65" symbol="NC"/>
<gate name="NC66" symbol="NC"/>
<gate name="NC67" symbol="NC"/>
<gate name="NC68" symbol="NC"/>
<gate name="NC69" symbol="NC"/>
<gate name="NC70" symbol="NC"/>
<gate name="NC71" symbol="NC"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="V24" symbol="VCCINT"/>
<gate name="V25" symbol="VCCINT"/>
<gate name="V26" symbol="VCCINT"/>
<gate name="V27" symbol="VCCINT"/>
<gate name="V28" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
<gate name="VO30" symbol="VCCIO"/>
<gate name="VO31" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="BGA672">
<connects>
<connect gate="-1" pin="IO11" pad="AF3"/>
<connect gate="-1" pin="IO12" pad="C6"/>
<connect gate="-1" pin="IO13" pad="A3"/>
<connect gate="-1" pin="IO14" pad="AC5"/>
<connect gate="-1" pin="IO21" pad="AE3"/>
<connect gate="-1" pin="IO22" pad="D5"/>
<connect gate="-1" pin="IO23" pad="B3"/>
<connect gate="-1" pin="IO24" pad="AC6"/>
<connect gate="-1" pin="IO31" pad="AD4"/>
<connect gate="-1" pin="IO32" pad="D6"/>
<connect gate="-1" pin="IO33" pad="C4"/>
<connect gate="-1" pin="IO34" pad="AA7"/>
<connect gate="-1" pin="IO41" pad="AD5"/>
<connect gate="-1" pin="IO42" pad="E7"/>
<connect gate="-1" pin="IO43" pad="C5"/>
<connect gate="-1" pin="IO44" pad="AD7"/>
<connect gate="-10" pin="IO371" pad="H16"/>
<connect gate="-10" pin="IO372" pad="G16"/>
<connect gate="-10" pin="IO373" pad="AF17"/>
<connect gate="-10" pin="IO374" pad="AD17"/>
<connect gate="-10" pin="IO381" pad="V16"/>
<connect gate="-10" pin="IO382" pad="D17"/>
<connect gate="-10" pin="IO383" pad="B17"/>
<connect gate="-10" pin="IO384" pad="AC17"/>
<connect gate="-10" pin="IO391" pad="AB17"/>
<connect gate="-10" pin="IO392" pad="C17"/>
<connect gate="-10" pin="IO393" pad="B18"/>
<connect gate="-10" pin="IO394" pad="AE18"/>
<connect gate="-10" pin="IO401" pad="J16"/>
<connect gate="-10" pin="IO402" pad="AC18"/>
<connect gate="-10" pin="IO403" pad="F17"/>
<connect gate="-10" pin="IO404" pad="Y17"/>
<connect gate="-11" pin="IO411" pad="AA17"/>
<connect gate="-11" pin="IO412" pad="C18"/>
<connect gate="-11" pin="IO413" pad="D18"/>
<connect gate="-11" pin="IO414" pad="AB19"/>
<connect gate="-11" pin="IO421" pad="AD19"/>
<connect gate="-11" pin="IO422" pad="H17"/>
<connect gate="-11" pin="IO423" pad="F18"/>
<connect gate="-11" pin="IO424" pad="AB18"/>
<connect gate="-11" pin="IO431" pad="AA18"/>
<connect gate="-11" pin="IO432" pad="E18"/>
<connect gate="-11" pin="IO433" pad="H18"/>
<connect gate="-11" pin="IO434" pad="AA19"/>
<connect gate="-11" pin="IO441" pad="AC20"/>
<connect gate="-11" pin="IO442" pad="G18"/>
<connect gate="-11" pin="IO443" pad="E19"/>
<connect gate="-11" pin="IO444" pad="AF19"/>
<connect gate="-12" pin="IO451" pad="AC19"/>
<connect gate="-12" pin="IO452" pad="F19"/>
<connect gate="-12" pin="IO453" pad="C20"/>
<connect gate="-12" pin="IO454" pad="AC21"/>
<connect gate="-12" pin="IO461" pad="AB20"/>
<connect gate="-12" pin="IO462" pad="E21"/>
<connect gate="-12" pin="IO463" pad="C19"/>
<connect gate="-12" pin="IO464" pad="AD20"/>
<connect gate="-12" pin="IO471" pad="AB21"/>
<connect gate="-12" pin="IO472" pad="C21"/>
<connect gate="-12" pin="IO473" pad="E20"/>
<connect gate="-12" pin="IO474" pad="AD21"/>
<connect gate="-12" pin="IO481" pad="AC22"/>
<connect gate="-12" pin="IO482" pad="C22"/>
<connect gate="-12" pin="IO483" pad="D20"/>
<connect gate="-12" pin="IO484" pad="AD22"/>
<connect gate="-13" pin="IO491" pad="AE26"/>
<connect gate="-13" pin="IO492" pad="H19"/>
<connect gate="-13" pin="IO493" pad="D21"/>
<connect gate="-13" pin="IO494" pad="AC23"/>
<connect gate="-13" pin="IO501" pad="D22"/>
<connect gate="-13" pin="IO502" pad="G19"/>
<connect gate="-13" pin="IO503" pad="AD26"/>
<connect gate="-13" pin="IO504" pad="AF22"/>
<connect gate="-13" pin="IO511" pad="AE24"/>
<connect gate="-13" pin="IO512" pad="F20"/>
<connect gate="-13" pin="IO513" pad="E22"/>
<connect gate="-13" pin="IO514" pad="AD23"/>
<connect gate="-13" pin="IO521" pad="AD25"/>
<connect gate="-13" pin="IO522" pad="F21"/>
<connect gate="-13" pin="IO523" pad="C23"/>
<connect gate="-13" pin="IO524" pad="AD24"/>
<connect gate="-2" pin="IO51" pad="W7"/>
<connect gate="-2" pin="IO52" pad="AD6"/>
<connect gate="-2" pin="IO53" pad="E8"/>
<connect gate="-2" pin="IO54" pad="E5"/>
<connect gate="-2" pin="IO61" pad="AA8"/>
<connect gate="-2" pin="IO62" pad="D8"/>
<connect gate="-2" pin="IO63" pad="E6"/>
<connect gate="-2" pin="IO64" pad="AB6"/>
<connect gate="-2" pin="IO71" pad="AB8"/>
<connect gate="-2" pin="IO72" pad="F8"/>
<connect gate="-2" pin="IO73" pad="C7"/>
<connect gate="-2" pin="IO74" pad="AB7"/>
<connect gate="-2" pin="IO81" pad="Y8"/>
<connect gate="-2" pin="IO82" pad="AC7"/>
<connect gate="-2" pin="IO83" pad="A8"/>
<connect gate="-2" pin="IO84" pad="A7"/>
<connect gate="-3" pin="IO101" pad="W8"/>
<connect gate="-3" pin="IO102" pad="F7"/>
<connect gate="-3" pin="IO103" pad="E9"/>
<connect gate="-3" pin="IO104" pad="AB9"/>
<connect gate="-3" pin="IO111" pad="W9"/>
<connect gate="-3" pin="IO112" pad="H8"/>
<connect gate="-3" pin="IO113" pad="D9"/>
<connect gate="-3" pin="IO114" pad="AD9"/>
<connect gate="-3" pin="IO121" pad="AA9"/>
<connect gate="-3" pin="IO122" pad="C9"/>
<connect gate="-3" pin="IO123" pad="G9"/>
<connect gate="-3" pin="IO124" pad="W10"/>
<connect gate="-3" pin="IO91" pad="AD8"/>
<connect gate="-3" pin="IO92" pad="G8"/>
<connect gate="-3" pin="IO93" pad="H10"/>
<connect gate="-3" pin="IO94" pad="Y9"/>
<connect gate="-4" pin="IO131" pad="AC9"/>
<connect gate="-4" pin="IO132" pad="F9"/>
<connect gate="-4" pin="IO133" pad="F10"/>
<connect gate="-4" pin="IO134" pad="AA10"/>
<connect gate="-4" pin="IO141" pad="V10"/>
<connect gate="-4" pin="IO142" pad="J9"/>
<connect gate="-4" pin="IO143" pad="A9"/>
<connect gate="-4" pin="IO144" pad="AC10"/>
<connect gate="-4" pin="IO151" pad="Y10"/>
<connect gate="-4" pin="IO152" pad="G10"/>
<connect gate="-4" pin="IO153" pad="E10"/>
<connect gate="-4" pin="IO154" pad="V11"/>
<connect gate="-4" pin="IO161" pad="AD10"/>
<connect gate="-4" pin="IO162" pad="D10"/>
<connect gate="-4" pin="IO163" pad="H11"/>
<connect gate="-4" pin="IO164" pad="W11"/>
<connect gate="-5" pin="IO171" pad="Y11"/>
<connect gate="-5" pin="IO172" pad="E11"/>
<connect gate="-5" pin="IO173" pad="G11"/>
<connect gate="-5" pin="IO174" pad="AA11"/>
<connect gate="-5" pin="IO181" pad="AC11"/>
<connect gate="-5" pin="IO182" pad="D11"/>
<connect gate="-5" pin="IO183" pad="F11"/>
<connect gate="-5" pin="IO184" pad="AB11"/>
<connect gate="-5" pin="IO191" pad="AD11"/>
<connect gate="-5" pin="IO192" pad="J11"/>
<connect gate="-5" pin="IO193" pad="C11"/>
<connect gate="-5" pin="IO194" pad="AF11"/>
<connect gate="-5" pin="IO201" pad="V12"/>
<connect gate="-5" pin="IO202" pad="G12"/>
<connect gate="-5" pin="IO203" pad="H12"/>
<connect gate="-5" pin="IO204" pad="U12"/>
<connect gate="-6" pin="IO211" pad="Y12"/>
<connect gate="-6" pin="IO212" pad="F12"/>
<connect gate="-6" pin="IO213" pad="D12"/>
<connect gate="-6" pin="IO214" pad="W12"/>
<connect gate="-6" pin="IO221" pad="AB12"/>
<connect gate="-6" pin="IO222" pad="E12"/>
<connect gate="-6" pin="IO223" pad="J12"/>
<connect gate="-6" pin="IO224" pad="AA12"/>
<connect gate="-6" pin="IO231" pad="AC12"/>
<connect gate="-6" pin="IO232" pad="C12"/>
<connect gate="-6" pin="IO233" pad="H13"/>
<connect gate="-6" pin="IO234" pad="AD12"/>
<connect gate="-6" pin="IO241" pad="U13"/>
<connect gate="-6" pin="IO242" pad="K12"/>
<connect gate="-6" pin="IO243" pad="G13"/>
<connect gate="-6" pin="IO244" pad="V13"/>
<connect gate="-7" pin="IO251" pad="F13"/>
<connect gate="-7" pin="IO252" pad="D13"/>
<connect gate="-7" pin="IO253" pad="AE13"/>
<connect gate="-7" pin="IO254" pad="W13"/>
<connect gate="-7" pin="IO261" pad="C13"/>
<connect gate="-7" pin="IO262" pad="J13"/>
<connect gate="-7" pin="IO263" pad="AB13"/>
<connect gate="-7" pin="IO264" pad="AC13"/>
<connect gate="-7" pin="IO271" pad="AA14"/>
<connect gate="-7" pin="IO272" pad="H14"/>
<connect gate="-7" pin="IO273" pad="E14"/>
<connect gate="-7" pin="IO274" pad="AD14"/>
<connect gate="-7" pin="IO281" pad="Y14"/>
<connect gate="-7" pin="IO282" pad="AB14"/>
<connect gate="-7" pin="IO283" pad="C14"/>
<connect gate="-7" pin="IO284" pad="B14"/>
<connect gate="-8" pin="IO291" pad="V14"/>
<connect gate="-8" pin="IO292" pad="J14"/>
<connect gate="-8" pin="IO293" pad="D14"/>
<connect gate="-8" pin="IO294" pad="W14"/>
<connect gate="-8" pin="IO301" pad="AC15"/>
<connect gate="-8" pin="IO302" pad="J15"/>
<connect gate="-8" pin="IO303" pad="K14"/>
<connect gate="-8" pin="IO304" pad="U15"/>
<connect gate="-8" pin="IO311" pad="AA15"/>
<connect gate="-8" pin="IO312" pad="B15"/>
<connect gate="-8" pin="IO313" pad="H15"/>
<connect gate="-8" pin="IO314" pad="AB15"/>
<connect gate="-8" pin="IO321" pad="W15"/>
<connect gate="-8" pin="IO322" pad="D15"/>
<connect gate="-8" pin="IO323" pad="E15"/>
<connect gate="-8" pin="IO324" pad="Y15"/>
<connect gate="-9" pin="IO331" pad="V15"/>
<connect gate="-9" pin="IO332" pad="G15"/>
<connect gate="-9" pin="IO333" pad="F15"/>
<connect gate="-9" pin="IO334" pad="AC16"/>
<connect gate="-9" pin="IO341" pad="AD16"/>
<connect gate="-9" pin="IO342" pad="C16"/>
<connect gate="-9" pin="IO343" pad="K15"/>
<connect gate="-9" pin="IO344" pad="AB16"/>
<connect gate="-9" pin="IO351" pad="AA16"/>
<connect gate="-9" pin="IO352" pad="D16"/>
<connect gate="-9" pin="IO353" pad="Y16"/>
<connect gate="-9" pin="IO354" pad="G17"/>
<connect gate="-9" pin="IO361" pad="W17"/>
<connect gate="-9" pin="IO362" pad="W16"/>
<connect gate="-9" pin="IO363" pad="E16"/>
<connect gate="-9" pin="IO364" pad="F16"/>
<connect gate="-A" pin="IOA1" pad="B26"/>
<connect gate="-A" pin="IOA10" pad="E3"/>
<connect gate="-A" pin="IOA11" pad="F5"/>
<connect gate="-A" pin="IOA2" pad="C26"/>
<connect gate="-A" pin="IOA3" pad="J20"/>
<connect gate="-A" pin="IOA4" pad="C2"/>
<connect gate="-A" pin="IOA5" pad="D2"/>
<connect gate="-A" pin="IOA6" pad="B1"/>
<connect gate="-A" pin="IOA7" pad="E24"/>
<connect gate="-A" pin="IOA8" pad="F4"/>
<connect gate="-A" pin="IOA9" pad="F22"/>
<connect gate="-B" pin="IOB1" pad="D25"/>
<connect gate="-B" pin="IOB10" pad="E2"/>
<connect gate="-B" pin="IOB11" pad="C25"/>
<connect gate="-B" pin="IOB2" pad="F23"/>
<connect gate="-B" pin="IOB3" pad="E1"/>
<connect gate="-B" pin="IOB4" pad="D1"/>
<connect gate="-B" pin="IOB5" pad="F2"/>
<connect gate="-B" pin="IOB6" pad="D26"/>
<connect gate="-B" pin="IOB7" pad="F24"/>
<connect gate="-B" pin="IOB8" pad="F3"/>
<connect gate="-B" pin="IOB9" pad="G22"/>
<connect gate="-C" pin="IOC1" pad="E26"/>
<connect gate="-C" pin="IOC10" pad="H22"/>
<connect gate="-C" pin="IOC2" pad="F25"/>
<connect gate="-C" pin="IOC3" pad="G1"/>
<connect gate="-C" pin="IOC4" pad="G4"/>
<connect gate="-C" pin="IOC5" pad="G5"/>
<connect gate="-C" pin="IOC6" pad="G24"/>
<connect gate="-C" pin="IOC7" pad="G2"/>
<connect gate="-C" pin="IOC8" pad="E25"/>
<connect gate="-C" pin="IOC9" pad="F1"/>
<connect gate="-D" pin="IOD1" pad="H23"/>
<connect gate="-D" pin="IOD10" pad="F26"/>
<connect gate="-D" pin="IOD11" pad="H5"/>
<connect gate="-D" pin="IOD2" pad="G26"/>
<connect gate="-D" pin="IOD3" pad="J10"/>
<connect gate="-D" pin="IOD4" pad="H4"/>
<connect gate="-D" pin="IOD5" pad="H6"/>
<connect gate="-D" pin="IOD6" pad="H24"/>
<connect gate="-D" pin="IOD7" pad="H9"/>
<connect gate="-D" pin="IOD8" pad="G25"/>
<connect gate="-D" pin="IOD9" pad="H3"/>
<connect gate="-E" pin="IOE1" pad="J22"/>
<connect gate="-E" pin="IOE11" pad="J19"/>
<connect gate="-E" pin="IOE2" pad="K9"/>
<connect gate="-E" pin="IOE3" pad="J6"/>
<connect gate="-E" pin="IOE4" pad="J7"/>
<connect gate="-E" pin="IOE5" pad="J8"/>
<connect gate="-E" pin="IOE6" pad="H26"/>
<connect gate="-E" pin="IOE7" pad="J18"/>
<connect gate="-E" pin="IOE8" pad="H1"/>
<connect gate="-E" pin="IOE9" pad="J21"/>
<connect gate="-F" pin="IOF1" pad="K21"/>
<connect gate="-F" pin="IOF10" pad="K8"/>
<connect gate="-F" pin="IOF2" pad="J25"/>
<connect gate="-F" pin="IOF3" pad="K7"/>
<connect gate="-F" pin="IOF5" pad="J4"/>
<connect gate="-F" pin="IOF6" pad="J24"/>
<connect gate="-F" pin="IOF7" pad="J1"/>
<connect gate="-F" pin="IOF8" pad="J2"/>
<connect gate="-F" pin="IOF9" pad="K20"/>
<connect gate="-G" pin="IOG1" pad="K23"/>
<connect gate="-G" pin="IOG10" pad="K18"/>
<connect gate="-G" pin="IOG11" pad="K2"/>
<connect gate="-G" pin="IOG2" pad="K5"/>
<connect gate="-G" pin="IOG3" pad="K1"/>
<connect gate="-G" pin="IOG4" pad="L18"/>
<connect gate="-G" pin="IOG5" pad="K6"/>
<connect gate="-G" pin="IOG6" pad="J26"/>
<connect gate="-G" pin="IOG7" pad="L9"/>
<connect gate="-G" pin="IOG8" pad="K19"/>
<connect gate="-G" pin="IOG9" pad="K3"/>
<connect gate="-H" pin="IOH1" pad="L6"/>
<connect gate="-H" pin="IOH10" pad="K24"/>
<connect gate="-H" pin="IOH11" pad="K26"/>
<connect gate="-H" pin="IOH2" pad="L8"/>
<connect gate="-H" pin="IOH3" pad="L7"/>
<connect gate="-H" pin="IOH4" pad="L5"/>
<connect gate="-H" pin="IOH5" pad="K25"/>
<connect gate="-H" pin="IOH6" pad="L21"/>
<connect gate="-H" pin="IOH7" pad="L20"/>
<connect gate="-H" pin="IOH8" pad="L19"/>
<connect gate="-H" pin="IOH9" pad="L2"/>
<connect gate="-I" pin="IOI1" pad="M19"/>
<connect gate="-I" pin="IOI10" pad="M18"/>
<connect gate="-I" pin="IOI11" pad="M10"/>
<connect gate="-I" pin="IOI2" pad="L23"/>
<connect gate="-I" pin="IOI3" pad="M9"/>
<connect gate="-I" pin="IOI4" pad="L25"/>
<connect gate="-I" pin="IOI5" pad="L3"/>
<connect gate="-I" pin="IOI6" pad="L1"/>
<connect gate="-I" pin="IOI7" pad="L24"/>
<connect gate="-I" pin="IOI8" pad="M17"/>
<connect gate="-I" pin="IOI9" pad="L4"/>
<connect gate="-J" pin="IOJ1" pad="L26"/>
<connect gate="-J" pin="IOJ10" pad="M24"/>
<connect gate="-J" pin="IOJ12" pad="M4"/>
<connect gate="-J" pin="IOJ13" pad="M20"/>
<connect gate="-J" pin="IOJ2" pad="M21"/>
<connect gate="-J" pin="IOJ3" pad="M1"/>
<connect gate="-J" pin="IOJ4" pad="M3"/>
<connect gate="-J" pin="IOJ5" pad="M6"/>
<connect gate="-J" pin="IOJ6" pad="M23"/>
<connect gate="-J" pin="IOJ7" pad="N10"/>
<connect gate="-J" pin="IOJ8" pad="N19"/>
<connect gate="-J" pin="IOJ9" pad="M8"/>
<connect gate="-K" pin="IOK1" pad="N23"/>
<connect gate="-K" pin="IOK10" pad="M7"/>
<connect gate="-K" pin="IOK11" pad="N21"/>
<connect gate="-K" pin="IOK2" pad="N22"/>
<connect gate="-K" pin="IOK3" pad="N3"/>
<connect gate="-K" pin="IOK4" pad="N1"/>
<connect gate="-K" pin="IOK5" pad="N2"/>
<connect gate="-K" pin="IOK6" pad="N9"/>
<connect gate="-K" pin="IOK7" pad="N20"/>
<connect gate="-K" pin="IOK8" pad="N18"/>
<connect gate="-K" pin="IOK9" pad="M26"/>
<connect gate="-L" pin="IOL1" pad="N25"/>
<connect gate="-L" pin="IOL10" pad="N5"/>
<connect gate="-L" pin="IOL2" pad="N26"/>
<connect gate="-L" pin="IOL3" pad="N8"/>
<connect gate="-L" pin="IOL4" pad="P19"/>
<connect gate="-L" pin="IOL5" pad="N4"/>
<connect gate="-L" pin="IOL6" pad="N6"/>
<connect gate="-L" pin="IOL7" pad="N7"/>
<connect gate="-L" pin="IOL8" pad="N17"/>
<connect gate="-L" pin="IOL9" pad="N24"/>
<connect gate="-M" pin="IOM1" pad="P24"/>
<connect gate="-M" pin="IOM10" pad="P2"/>
<connect gate="-M" pin="IOM11" pad="P21"/>
<connect gate="-M" pin="IOM2" pad="P23"/>
<connect gate="-M" pin="IOM3" pad="P6"/>
<connect gate="-M" pin="IOM4" pad="P5"/>
<connect gate="-M" pin="IOM5" pad="P3"/>
<connect gate="-M" pin="IOM6" pad="P4"/>
<connect gate="-M" pin="IOM7" pad="P25"/>
<connect gate="-M" pin="IOM8" pad="P20"/>
<connect gate="-M" pin="IOM9" pad="P1"/>
<connect gate="-N" pin="ION1" pad="P18"/>
<connect gate="-N" pin="ION10" pad="P17"/>
<connect gate="-N" pin="ION11" pad="R20"/>
<connect gate="-N" pin="ION2" pad="R23"/>
<connect gate="-N" pin="ION3" pad="P9"/>
<connect gate="-N" pin="ION4" pad="P8"/>
<connect gate="-N" pin="ION5" pad="R1"/>
<connect gate="-N" pin="ION6" pad="P26"/>
<connect gate="-N" pin="ION7" pad="P7"/>
<connect gate="-N" pin="ION8" pad="R2"/>
<connect gate="-N" pin="ION9" pad="R21"/>
<connect gate="-O" pin="IOO1" pad="R26"/>
<connect gate="-O" pin="IOO10" pad="R24"/>
<connect gate="-O" pin="IOO2" pad="P10"/>
<connect gate="-O" pin="IOO3" pad="R7"/>
<connect gate="-O" pin="IOO4" pad="R4"/>
<connect gate="-O" pin="IOO5" pad="R17"/>
<connect gate="-O" pin="IOO6" pad="R6"/>
<connect gate="-O" pin="IOO7" pad="R25"/>
<connect gate="-O" pin="IOO8" pad="R19"/>
<connect gate="-O" pin="IOO9" pad="R3"/>
<connect gate="-P" pin="IOP1" pad="R18"/>
<connect gate="-P" pin="IOP10" pad="T22"/>
<connect gate="-P" pin="IOP11" pad="T24"/>
<connect gate="-P" pin="IOP2" pad="R9"/>
<connect gate="-P" pin="IOP3" pad="T3"/>
<connect gate="-P" pin="IOP4" pad="T4"/>
<connect gate="-P" pin="IOP5" pad="T23"/>
<connect gate="-P" pin="IOP6" pad="R8"/>
<connect gate="-P" pin="IOP7" pad="T5"/>
<connect gate="-P" pin="IOP8" pad="T21"/>
<connect gate="-P" pin="IOP9" pad="T1"/>
<connect gate="-Q" pin="IOQ1" pad="T19"/>
<connect gate="-Q" pin="IOQ10" pad="T20"/>
<connect gate="-Q" pin="IOQ11" pad="U21"/>
<connect gate="-Q" pin="IOQ2" pad="U2"/>
<connect gate="-Q" pin="IOQ3" pad="U1"/>
<connect gate="-Q" pin="IOQ4" pad="U25"/>
<connect gate="-Q" pin="IOQ5" pad="T26"/>
<connect gate="-Q" pin="IOQ6" pad="T7"/>
<connect gate="-Q" pin="IOQ7" pad="U22"/>
<connect gate="-Q" pin="IOQ8" pad="R10"/>
<connect gate="-Q" pin="IOQ9" pad="T6"/>
<connect gate="-R" pin="IOR1" pad="U20"/>
<connect gate="-R" pin="IOR10" pad="T18"/>
<connect gate="-R" pin="IOR2" pad="U26"/>
<connect gate="-R" pin="IOR3" pad="U23"/>
<connect gate="-R" pin="IOR4" pad="U5"/>
<connect gate="-R" pin="IOR5" pad="T9"/>
<connect gate="-R" pin="IOR6" pad="U18"/>
<connect gate="-R" pin="IOR7" pad="T8"/>
<connect gate="-R" pin="IOR8" pad="U6"/>
<connect gate="-R" pin="IOR9" pad="U4"/>
<connect gate="-S" pin="IOS1" pad="V18"/>
<connect gate="-S" pin="IOS10" pad="V19"/>
<connect gate="-S" pin="IOS11" pad="U19"/>
<connect gate="-S" pin="IOS2" pad="V23"/>
<connect gate="-S" pin="IOS3" pad="U8"/>
<connect gate="-S" pin="IOS4" pad="U9"/>
<connect gate="-S" pin="IOS5" pad="U7"/>
<connect gate="-S" pin="IOS6" pad="V22"/>
<connect gate="-S" pin="IOS7" pad="V2"/>
<connect gate="-S" pin="IOS8" pad="V4"/>
<connect gate="-S" pin="IOS9" pad="V1"/>
<connect gate="-T" pin="IOT1" pad="W23"/>
<connect gate="-T" pin="IOT10" pad="V21"/>
<connect gate="-T" pin="IOT11" pad="V26"/>
<connect gate="-T" pin="IOT2" pad="W1"/>
<connect gate="-T" pin="IOT3" pad="V7"/>
<connect gate="-T" pin="IOT4" pad="W3"/>
<connect gate="-T" pin="IOT5" pad="Y18"/>
<connect gate="-T" pin="IOT6" pad="V25"/>
<connect gate="-T" pin="IOT7" pad="W2"/>
<connect gate="-T" pin="IOT8" pad="W18"/>
<connect gate="-T" pin="IOT9" pad="V6"/>
<connect gate="-U" pin="IOU1" pad="W25"/>
<connect gate="-U" pin="IOU10" pad="W24"/>
<connect gate="-U" pin="IOU2" pad="W22"/>
<connect gate="-U" pin="IOU3" pad="V8"/>
<connect gate="-U" pin="IOU4" pad="W5"/>
<connect gate="-U" pin="IOU5" pad="Y3"/>
<connect gate="-U" pin="IOU6" pad="W19"/>
<connect gate="-U" pin="IOU7" pad="W4"/>
<connect gate="-U" pin="IOU8" pad="Y1"/>
<connect gate="-U" pin="IOU9" pad="W26"/>
<connect gate="-V" pin="IOV1" pad="Y25"/>
<connect gate="-V" pin="IOV10" pad="W21"/>
<connect gate="-V" pin="IOV11" pad="AA1"/>
<connect gate="-V" pin="IOV2" pad="Y19"/>
<connect gate="-V" pin="IOV3" pad="AB2"/>
<connect gate="-V" pin="IOV4" pad="Y4"/>
<connect gate="-V" pin="IOV5" pad="AA3"/>
<connect gate="-V" pin="IOV6" pad="V20"/>
<connect gate="-V" pin="IOV7" pad="AB1"/>
<connect gate="-V" pin="IOV8" pad="AA20"/>
<connect gate="-V" pin="IOV9" pad="AA2"/>
<connect gate="-W" pin="IOW1" pad="Y22"/>
<connect gate="-W" pin="IOW10" pad="Y26"/>
<connect gate="-W" pin="IOW11" pad="AA25"/>
<connect gate="-W" pin="IOW2" pad="AD2"/>
<connect gate="-W" pin="IOW3" pad="AA4"/>
<connect gate="-W" pin="IOW4" pad="AB26"/>
<connect gate="-W" pin="IOW5" pad="AC2"/>
<connect gate="-W" pin="IOW6" pad="Y23"/>
<connect gate="-W" pin="IOW7" pad="AD1"/>
<connect gate="-W" pin="IOW8" pad="Y20"/>
<connect gate="-W" pin="IOW9" pad="AC1"/>
<connect gate="-X" pin="IOX1" pad="AA24"/>
<connect gate="-X" pin="IOX10" pad="AC26"/>
<connect gate="-X" pin="IOX2" pad="AC25"/>
<connect gate="-X" pin="IOX3" pad="AD3"/>
<connect gate="-X" pin="IOX4" pad="AA6"/>
<connect gate="-X" pin="IOX5" pad="AC4"/>
<connect gate="-X" pin="IOX6" pad="AB22"/>
<connect gate="-X" pin="IOX7" pad="AB25"/>
<connect gate="-X" pin="IOX8" pad="AE1"/>
<connect gate="-X" pin="IOX9" pad="AA5"/>
<connect gate="G1" pin="GND" pad="AA13"/>
<connect gate="G10" pin="GND" pad="AC24"/>
<connect gate="G11" pin="GND" pad="AD13"/>
<connect gate="G12" pin="GND" pad="AD18"/>
<connect gate="G13" pin="GND" pad="AE2"/>
<connect gate="G14" pin="GND" pad="AE25"/>
<connect gate="G15" pin="GND" pad="AF2"/>
<connect gate="G16" pin="GND" pad="AF25"/>
<connect gate="G17" pin="GND" pad="A2"/>
<connect gate="G18" pin="GND" pad="A25"/>
<connect gate="G19" pin="GND" pad="B2"/>
<connect gate="G2" pin="GND" pad="AA22"/>
<connect gate="G20" pin="GND" pad="B25"/>
<connect gate="G21" pin="GND" pad="C3"/>
<connect gate="G22" pin="GND" pad="C10"/>
<connect gate="G23" pin="GND" pad="C24"/>
<connect gate="G24" pin="GND" pad="D3"/>
<connect gate="G25" pin="GND" pad="D4"/>
<connect gate="G26" pin="GND" pad="D19"/>
<connect gate="G27" pin="GND" pad="D23"/>
<connect gate="G28" pin="GND" pad="D24"/>
<connect gate="G29" pin="GND" pad="E4"/>
<connect gate="G3" pin="GND" pad="AB3"/>
<connect gate="G30" pin="GND" pad="E23"/>
<connect gate="G31" pin="GND" pad="G23"/>
<connect gate="G32" pin="GND" pad="J5"/>
<connect gate="G33" pin="GND" pad="J23"/>
<connect gate="G34" pin="GND" pad="K4"/>
<connect gate="G35" pin="GND" pad="K10"/>
<connect gate="G36" pin="GND" pad="K17"/>
<connect gate="G37" pin="GND" pad="L11"/>
<connect gate="G38" pin="GND" pad="L16"/>
<connect gate="G39" pin="GND" pad="L22"/>
<connect gate="G4" pin="GND" pad="AB4"/>
<connect gate="G40" pin="GND" pad="M5"/>
<connect gate="G41" pin="GND" pad="M12"/>
<connect gate="G42" pin="GND" pad="M14"/>
<connect gate="G43" pin="GND" pad="M15"/>
<connect gate="G44" pin="GND" pad="N13"/>
<connect gate="G45" pin="GND" pad="N14"/>
<connect gate="G46" pin="GND" pad="P13"/>
<connect gate="G47" pin="GND" pad="P14"/>
<connect gate="G48" pin="GND" pad="P22"/>
<connect gate="G49" pin="GND" pad="R12"/>
<connect gate="G5" pin="GND" pad="AB5"/>
<connect gate="G50" pin="GND" pad="R15"/>
<connect gate="G51" pin="GND" pad="T11"/>
<connect gate="G52" pin="GND" pad="T16"/>
<connect gate="G53" pin="GND" pad="U10"/>
<connect gate="G54" pin="GND" pad="U17"/>
<connect gate="G55" pin="GND" pad="U24"/>
<connect gate="G56" pin="GND" pad="V3"/>
<connect gate="G57" pin="GND" pad="Y5"/>
<connect gate="G6" pin="GND" pad="AB23"/>
<connect gate="G7" pin="GND" pad="AB24"/>
<connect gate="G8" pin="GND" pad="AC3"/>
<connect gate="G9" pin="GND" pad="AC8"/>
<connect gate="NC1" pin="NC" pad="AE4"/>
<connect gate="NC10" pin="NC" pad="AE14"/>
<connect gate="NC11" pin="NC" pad="AE15"/>
<connect gate="NC12" pin="NC" pad="AE16"/>
<connect gate="NC13" pin="NC" pad="AE17"/>
<connect gate="NC14" pin="NC" pad="AE19"/>
<connect gate="NC15" pin="NC" pad="AE20"/>
<connect gate="NC16" pin="NC" pad="AE21"/>
<connect gate="NC17" pin="NC" pad="AE22"/>
<connect gate="NC18" pin="NC" pad="AE23"/>
<connect gate="NC19" pin="NC" pad="AF4"/>
<connect gate="NC2" pin="NC" pad="AE5"/>
<connect gate="NC20" pin="NC" pad="AF5"/>
<connect gate="NC21" pin="NC" pad="AF6"/>
<connect gate="NC22" pin="NC" pad="AF7"/>
<connect gate="NC23" pin="NC" pad="AF8"/>
<connect gate="NC24" pin="NC" pad="AF9"/>
<connect gate="NC25" pin="NC" pad="AF10"/>
<connect gate="NC26" pin="NC" pad="AF12"/>
<connect gate="NC27" pin="NC" pad="AF13"/>
<connect gate="NC28" pin="NC" pad="AF14"/>
<connect gate="NC29" pin="NC" pad="AF15"/>
<connect gate="NC3" pin="NC" pad="AE6"/>
<connect gate="NC30" pin="NC" pad="AF16"/>
<connect gate="NC31" pin="NC" pad="AF18"/>
<connect gate="NC32" pin="NC" pad="AF20"/>
<connect gate="NC33" pin="NC" pad="AF21"/>
<connect gate="NC34" pin="NC" pad="AF23"/>
<connect gate="NC35" pin="NC" pad="AF24"/>
<connect gate="NC36" pin="NC" pad="A4"/>
<connect gate="NC37" pin="NC" pad="A5"/>
<connect gate="NC38" pin="NC" pad="A6"/>
<connect gate="NC39" pin="NC" pad="A10"/>
<connect gate="NC4" pin="NC" pad="AE7"/>
<connect gate="NC40" pin="NC" pad="A11"/>
<connect gate="NC41" pin="NC" pad="A12"/>
<connect gate="NC42" pin="NC" pad="A13"/>
<connect gate="NC43" pin="NC" pad="A14"/>
<connect gate="NC44" pin="NC" pad="A15"/>
<connect gate="NC45" pin="NC" pad="A16"/>
<connect gate="NC46" pin="NC" pad="A17"/>
<connect gate="NC47" pin="NC" pad="A18"/>
<connect gate="NC48" pin="NC" pad="A19"/>
<connect gate="NC49" pin="NC" pad="A20"/>
<connect gate="NC5" pin="NC" pad="AE8"/>
<connect gate="NC50" pin="NC" pad="A21"/>
<connect gate="NC51" pin="NC" pad="A22"/>
<connect gate="NC52" pin="NC" pad="A23"/>
<connect gate="NC53" pin="NC" pad="A24"/>
<connect gate="NC54" pin="NC" pad="B4"/>
<connect gate="NC55" pin="NC" pad="B5"/>
<connect gate="NC56" pin="NC" pad="B6"/>
<connect gate="NC57" pin="NC" pad="B7"/>
<connect gate="NC58" pin="NC" pad="B8"/>
<connect gate="NC59" pin="NC" pad="B9"/>
<connect gate="NC6" pin="NC" pad="AE9"/>
<connect gate="NC60" pin="NC" pad="B10"/>
<connect gate="NC61" pin="NC" pad="B11"/>
<connect gate="NC62" pin="NC" pad="B12"/>
<connect gate="NC63" pin="NC" pad="B13"/>
<connect gate="NC64" pin="NC" pad="B16"/>
<connect gate="NC65" pin="NC" pad="B19"/>
<connect gate="NC66" pin="NC" pad="B20"/>
<connect gate="NC67" pin="NC" pad="B21"/>
<connect gate="NC68" pin="NC" pad="B22"/>
<connect gate="NC69" pin="NC" pad="B23"/>
<connect gate="NC7" pin="NC" pad="AE10"/>
<connect gate="NC70" pin="NC" pad="B24"/>
<connect gate="NC71" pin="NC" pad="C1"/>
<connect gate="NC8" pin="NC" pad="AE11"/>
<connect gate="NC9" pin="NC" pad="AE12"/>
<connect gate="V1" pin="VCC" pad="AA23"/>
<connect gate="V10" pin="VCC" pad="L12"/>
<connect gate="V11" pin="VCC" pad="L14"/>
<connect gate="V12" pin="VCC" pad="L17"/>
<connect gate="V13" pin="VCC" pad="M2"/>
<connect gate="V14" pin="VCC" pad="M25"/>
<connect gate="V15" pin="VCC" pad="N11"/>
<connect gate="V16" pin="VCC" pad="N12"/>
<connect gate="V17" pin="VCC" pad="N15"/>
<connect gate="V18" pin="VCC" pad="P12"/>
<connect gate="V19" pin="VCC" pad="P15"/>
<connect gate="V2" pin="VCC" pad="AB10"/>
<connect gate="V20" pin="VCC" pad="P16"/>
<connect gate="V21" pin="VCC" pad="R14"/>
<connect gate="V22" pin="VCC" pad="T2"/>
<connect gate="V23" pin="VCC" pad="T10"/>
<connect gate="V24" pin="VCC" pad="T12"/>
<connect gate="V25" pin="VCC" pad="T17"/>
<connect gate="V26" pin="VCC" pad="T25"/>
<connect gate="V27" pin="VCC" pad="U16"/>
<connect gate="V28" pin="VCC" pad="Y7"/>
<connect gate="V3" pin="VCC" pad="AC14"/>
<connect gate="V4" pin="VCC" pad="E13"/>
<connect gate="V5" pin="VCC" pad="E17"/>
<connect gate="V6" pin="VCC" pad="H2"/>
<connect gate="V7" pin="VCC" pad="H25"/>
<connect gate="V8" pin="VCC" pad="K16"/>
<connect gate="V9" pin="VCC" pad="L10"/>
<connect gate="VO1" pin="VCCIO" pad="AA26"/>
<connect gate="VO10" pin="VCCIO" pad="K22"/>
<connect gate="VO11" pin="VCCIO" pad="L13"/>
<connect gate="VO12" pin="VCCIO" pad="L15"/>
<connect gate="VO13" pin="VCCIO" pad="M11"/>
<connect gate="VO14" pin="VCCIO" pad="M13"/>
<connect gate="VO15" pin="VCCIO" pad="M16"/>
<connect gate="VO16" pin="VCCIO" pad="M22"/>
<connect gate="VO17" pin="VCCIO" pad="N16"/>
<connect gate="VO18" pin="VCCIO" pad="P11"/>
<connect gate="VO19" pin="VCCIO" pad="R5"/>
<connect gate="VO2" pin="VCCIO" pad="AD15"/>
<connect gate="VO20" pin="VCCIO" pad="R11"/>
<connect gate="VO21" pin="VCCIO" pad="R13"/>
<connect gate="VO22" pin="VCCIO" pad="R16"/>
<connect gate="VO23" pin="VCCIO" pad="R22"/>
<connect gate="VO24" pin="VCCIO" pad="T15"/>
<connect gate="VO25" pin="VCCIO" pad="U3"/>
<connect gate="VO26" pin="VCCIO" pad="U11"/>
<connect gate="VO27" pin="VCCIO" pad="V5"/>
<connect gate="VO28" pin="VCCIO" pad="V17"/>
<connect gate="VO29" pin="VCCIO" pad="V24"/>
<connect gate="VO3" pin="VCCIO" pad="C8"/>
<connect gate="VO30" pin="VCCIO" pad="Y2"/>
<connect gate="VO31" pin="VCCIO" pad="Y24"/>
<connect gate="VO4" pin="VCCIO" pad="C15"/>
<connect gate="VO5" pin="VCCIO" pad="D7"/>
<connect gate="VO6" pin="VCCIO" pad="G3"/>
<connect gate="VO7" pin="VCCIO" pad="J3"/>
<connect gate="VO8" pin="VCCIO" pad="J17"/>
<connect gate="VO9" pin="VCCIO" pad="K11"/>
<connect gate="_" pin="/CE" pad="G6"/>
<connect gate="_" pin="/CEO" pad="G21"/>
<connect gate="_" pin="/CONFIG" pad="V9"/>
<connect gate="_" pin="/STATUS" pad="AA21"/>
<connect gate="_" pin="CONF_DONE" pad="H20"/>
<connect gate="_" pin="DATA0" pad="F6"/>
<connect gate="_" pin="DCLK" pad="G7"/>
<connect gate="_" pin="GCLK" pad="F14"/>
<connect gate="_" pin="GCLK1" pad="T13"/>
<connect gate="_" pin="IN0" pad="U14"/>
<connect gate="_" pin="IN1" pad="Y13"/>
<connect gate="_" pin="IN2" pad="K13"/>
<connect gate="_" pin="IN3" pad="G14"/>
<connect gate="_" pin="MSEL0" pad="W6"/>
<connect gate="_" pin="MSEL1" pad="Y6"/>
<connect gate="_" pin="TCK" pad="G20"/>
<connect gate="_" pin="TDI" pad="H7"/>
<connect gate="_" pin="TDO" pad="H21"/>
<connect gate="_" pin="TMS" pad="W20"/>
<connect gate="_" pin="TRST" pad="Y21"/>
<connect gate="_" pin="VCC_CKLK" pad="T14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K200EFC672-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8900"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K250-P599" prefix="IC">
<description>&lt;b&gt;EPF10K250&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="-0" symbol="K250_C"/>
<gate name="-A" symbol="A13-250"/>
<gate name="-B" symbol="B12-250"/>
<gate name="-C" symbol="C13-250"/>
<gate name="-D" symbol="D13-250"/>
<gate name="-E" symbol="E12-250"/>
<gate name="-F" symbol="F12-250"/>
<gate name="-G" symbol="G13-250"/>
<gate name="-H" symbol="H12-250"/>
<gate name="-I" symbol="I13-250"/>
<gate name="-J" symbol="J13-250"/>
<gate name="-K" symbol="K12-250"/>
<gate name="-L" symbol="L12-250"/>
<gate name="-M" symbol="M13-250"/>
<gate name="-N" symbol="N13-250"/>
<gate name="-O" symbol="O13-250"/>
<gate name="-Q" symbol="Q14-250"/>
<gate name="-S" symbol="S13-250"/>
<gate name="-T" symbol="T14-250"/>
<gate name="-1" symbol="62-250"/>
<gate name="-2" symbol="122-250"/>
<gate name="-3" symbol="182-250"/>
<gate name="-4" symbol="242-250"/>
<gate name="-5" symbol="302-250"/>
<gate name="-6" symbol="361-250"/>
<gate name="-7" symbol="412-250"/>
<gate name="-8" symbol="471-250"/>
<gate name="-9" symbol="531-250"/>
<gate name="-10" symbol="583-250"/>
<gate name="-11" symbol="642-250"/>
<gate name="-12" symbol="702-250"/>
<gate name="-13" symbol="762-250"/>
<gate name="-P" symbol="P14-250"/>
<gate name="-R" symbol="R12-250"/>
<gate name="GI1" symbol="GNDINT"/>
<gate name="GI2" symbol="GNDINT"/>
<gate name="GI3" symbol="GNDINT"/>
<gate name="GI4" symbol="GNDINT"/>
<gate name="GI5" symbol="GNDINT"/>
<gate name="GI6" symbol="GNDINT"/>
<gate name="GI7" symbol="GNDINT"/>
<gate name="GI8" symbol="GNDINT"/>
<gate name="GI9" symbol="GNDINT"/>
<gate name="GI10" symbol="GNDINT"/>
<gate name="GI11" symbol="GNDINT"/>
<gate name="GI12" symbol="GNDINT"/>
<gate name="GI13" symbol="GNDINT"/>
<gate name="GI14" symbol="GNDINT"/>
<gate name="GI15" symbol="GNDINT"/>
<gate name="GI16" symbol="GNDINT"/>
<gate name="GI17" symbol="GNDINT"/>
<gate name="GI18" symbol="GNDINT"/>
<gate name="GI19" symbol="GNDINT"/>
<gate name="GI20" symbol="GNDINT"/>
<gate name="GI21" symbol="GNDINT"/>
<gate name="GI22" symbol="GNDINT"/>
<gate name="GI23" symbol="GNDINT"/>
<gate name="GI24" symbol="GNDINT"/>
<gate name="GI25" symbol="GNDINT"/>
<gate name="GI26" symbol="GNDINT"/>
<gate name="GO1" symbol="GNDIO"/>
<gate name="GO2" symbol="GNDIO"/>
<gate name="GO3" symbol="GNDIO"/>
<gate name="GO4" symbol="GNDIO"/>
<gate name="GO5" symbol="GNDIO"/>
<gate name="GO6" symbol="GNDIO"/>
<gate name="GO7" symbol="GNDIO"/>
<gate name="GO8" symbol="GNDIO"/>
<gate name="GO9" symbol="GNDIO"/>
<gate name="GO10" symbol="GNDIO"/>
<gate name="GO11" symbol="GNDIO"/>
<gate name="GO12" symbol="GNDIO"/>
<gate name="GO13" symbol="GNDIO"/>
<gate name="GO14" symbol="GNDIO"/>
<gate name="GO15" symbol="GNDIO"/>
<gate name="GO16" symbol="GNDIO"/>
<gate name="GO17" symbol="GNDIO"/>
<gate name="GO18" symbol="GNDIO"/>
<gate name="GO19" symbol="GNDIO"/>
<gate name="GO20" symbol="GNDIO"/>
<gate name="GO21" symbol="GNDIO"/>
<gate name="GO22" symbol="GNDIO"/>
<gate name="GO23" symbol="GNDIO"/>
<gate name="GO24" symbol="GNDIO"/>
<gate name="GO25" symbol="GNDIO"/>
<gate name="GO26" symbol="GNDIO"/>
<gate name="GO27" symbol="GNDIO"/>
<gate name="GO28" symbol="GNDIO"/>
<gate name="GO29" symbol="GNDIO"/>
<gate name="GO30" symbol="GNDIO"/>
<gate name="GO31" symbol="GNDIO"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="V24" symbol="VCCINT"/>
<gate name="V25" symbol="VCCINT"/>
<gate name="V26" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
<gate name="VO30" symbol="VCCIO"/>
<gate name="VO31" symbol="VCCIO"/>
<gate name="VO32" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="PGA599">
<connects>
<connect gate="-0" pin="/CE" pad="BB6"/>
<connect gate="-0" pin="/CEO" pad="BF44"/>
<connect gate="-0" pin="/CONFIG" pad="B4"/>
<connect gate="-0" pin="/STATUS" pad="E43"/>
<connect gate="-0" pin="CONF_DONE" pad="BC43"/>
<connect gate="-0" pin="DATA0" pad="BC5"/>
<connect gate="-0" pin="DCLK" pad="BE5"/>
<connect gate="-0" pin="GCLK0" pad="A25"/>
<connect gate="-0" pin="GCLK1" pad="BF24"/>
<connect gate="-0" pin="IN0" pad="BG23"/>
<connect gate="-0" pin="IN1" pad="BG25"/>
<connect gate="-0" pin="IN2" pad="B24"/>
<connect gate="-0" pin="IN3" pad="C25"/>
<connect gate="-0" pin="MSEL0" pad="F6"/>
<connect gate="-0" pin="MSEL1" pad="C3"/>
<connect gate="-0" pin="TCK" pad="BE43"/>
<connect gate="-0" pin="TDI" pad="BF4"/>
<connect gate="-0" pin="TDO" pad="BB42"/>
<connect gate="-0" pin="TMS" pad="F42"/>
<connect gate="-0" pin="TRST" pad="B46"/>
<connect gate="-1" pin="IO11" pad="AY10"/>
<connect gate="-1" pin="IO12" pad="G9"/>
<connect gate="-1" pin="IO21" pad="BA9"/>
<connect gate="-1" pin="IO22" pad="BD6"/>
<connect gate="-1" pin="IO23" pad="C5"/>
<connect gate="-1" pin="IO31" pad="BF6"/>
<connect gate="-1" pin="IO32" pad="B6"/>
<connect gate="-1" pin="IO33" pad="F8"/>
<connect gate="-1" pin="IO41" pad="BB8"/>
<connect gate="-1" pin="IO42" pad="BD8"/>
<connect gate="-1" pin="IO43" pad="D6"/>
<connect gate="-1" pin="IO51" pad="BA11"/>
<connect gate="-1" pin="IO52" pad="D8"/>
<connect gate="-1" pin="IO53" pad="G11"/>
<connect gate="-1" pin="IO61" pad="BE7"/>
<connect gate="-1" pin="IO62" pad="C7"/>
<connect gate="-10" pin="IO532" pad="F30"/>
<connect gate="-10" pin="IO541" pad="BD32"/>
<connect gate="-10" pin="IO542" pad="BG33"/>
<connect gate="-10" pin="IO543" pad="B34"/>
<connect gate="-10" pin="IO551" pad="A35"/>
<connect gate="-10" pin="IO552" pad="BD34"/>
<connect gate="-10" pin="IO553" pad="D34"/>
<connect gate="-10" pin="IO561" pad="BA31"/>
<connect gate="-10" pin="IO562" pad="BE33"/>
<connect gate="-10" pin="IO563" pad="G31"/>
<connect gate="-10" pin="IO571" pad="BF34"/>
<connect gate="-10" pin="IO572" pad="B36"/>
<connect gate="-10" pin="IO573" pad="F32"/>
<connect gate="-10" pin="IO581" pad="A37"/>
<connect gate="-10" pin="IO582" pad="BB32"/>
<connect gate="-10" pin="IO583" pad="BG35"/>
<connect gate="-11" pin="IO591" pad="A39"/>
<connect gate="-11" pin="IO592" pad="BF36"/>
<connect gate="-11" pin="IO601" pad="BD36"/>
<connect gate="-11" pin="IO602" pad="BG37"/>
<connect gate="-11" pin="IO603" pad="D36"/>
<connect gate="-11" pin="IO611" pad="BB34"/>
<connect gate="-11" pin="IO612" pad="B38"/>
<connect gate="-11" pin="IO613" pad="F34"/>
<connect gate="-11" pin="IO621" pad="A41"/>
<connect gate="-11" pin="IO622" pad="BA33"/>
<connect gate="-11" pin="IO623" pad="BG39"/>
<connect gate="-11" pin="IO631" pad="BF38"/>
<connect gate="-11" pin="IO632" pad="B40"/>
<connect gate="-11" pin="IO633" pad="G33"/>
<connect gate="-11" pin="IO641" pad="BD38"/>
<connect gate="-11" pin="IO642" pad="D38"/>
<connect gate="-12" pin="IO651" pad="BB36"/>
<connect gate="-12" pin="IO652" pad="E37"/>
<connect gate="-12" pin="IO661" pad="BA35"/>
<connect gate="-12" pin="IO662" pad="BG41"/>
<connect gate="-12" pin="IO663" pad="G35"/>
<connect gate="-12" pin="IO671" pad="BF40"/>
<connect gate="-12" pin="IO672" pad="C39"/>
<connect gate="-12" pin="IO673" pad="F36"/>
<connect gate="-12" pin="IO681" pad="BC37"/>
<connect gate="-12" pin="IO682" pad="BE39"/>
<connect gate="-12" pin="IO683" pad="D40"/>
<connect gate="-12" pin="IO691" pad="A43"/>
<connect gate="-12" pin="IO692" pad="BB38"/>
<connect gate="-12" pin="IO693" pad="F38"/>
<connect gate="-12" pin="IO701" pad="BG43"/>
<connect gate="-12" pin="IO702" pad="B42"/>
<connect gate="-13" pin="IO711" pad="BE41"/>
<connect gate="-13" pin="IO712" pad="G37"/>
<connect gate="-13" pin="IO721" pad="BA37"/>
<connect gate="-13" pin="IO722" pad="BD40"/>
<connect gate="-13" pin="IO723" pad="D42"/>
<connect gate="-13" pin="IO731" pad="BB40"/>
<connect gate="-13" pin="IO732" pad="C41"/>
<connect gate="-13" pin="IO733" pad="F40"/>
<connect gate="-13" pin="IO741" pad="BA39"/>
<connect gate="-13" pin="IO742" pad="BF42"/>
<connect gate="-13" pin="IO743" pad="B44"/>
<connect gate="-13" pin="IO751" pad="BD42"/>
<connect gate="-13" pin="IO752" pad="C43"/>
<connect gate="-13" pin="IO753" pad="G39"/>
<connect gate="-13" pin="IO761" pad="AY38"/>
<connect gate="-13" pin="IO762" pad="H38"/>
<connect gate="-2" pin="IO101" pad="BA13"/>
<connect gate="-2" pin="IO102" pad="BF8"/>
<connect gate="-2" pin="IO103" pad="B8"/>
<connect gate="-2" pin="IO111" pad="A7"/>
<connect gate="-2" pin="IO112" pad="BG7"/>
<connect gate="-2" pin="IO113" pad="G13"/>
<connect gate="-2" pin="IO121" pad="BB12"/>
<connect gate="-2" pin="IO122" pad="F12"/>
<connect gate="-2" pin="IO71" pad="A5"/>
<connect gate="-2" pin="IO72" pad="BG5"/>
<connect gate="-2" pin="IO81" pad="BB10"/>
<connect gate="-2" pin="IO82" pad="BE9"/>
<connect gate="-2" pin="IO83" pad="F10"/>
<connect gate="-2" pin="IO91" pad="BC11"/>
<connect gate="-2" pin="IO92" pad="C9"/>
<connect gate="-2" pin="IO93" pad="E11"/>
<connect gate="-3" pin="IO131" pad="BD10"/>
<connect gate="-3" pin="IO132" pad="D10"/>
<connect gate="-3" pin="IO141" pad="BA15"/>
<connect gate="-3" pin="IO142" pad="BF10"/>
<connect gate="-3" pin="IO143" pad="B10"/>
<connect gate="-3" pin="IO151" pad="A9"/>
<connect gate="-3" pin="IO152" pad="BG9"/>
<connect gate="-3" pin="IO153" pad="G15"/>
<connect gate="-3" pin="IO161" pad="BB14"/>
<connect gate="-3" pin="IO162" pad="BG11"/>
<connect gate="-3" pin="IO163" pad="F14"/>
<connect gate="-3" pin="IO171" pad="A11"/>
<connect gate="-3" pin="IO172" pad="BD12"/>
<connect gate="-3" pin="IO173" pad="D12"/>
<connect gate="-3" pin="IO181" pad="BF12"/>
<connect gate="-3" pin="IO182" pad="B12"/>
<connect gate="-4" pin="IO191" pad="A13"/>
<connect gate="-4" pin="IO192" pad="BG13"/>
<connect gate="-4" pin="IO201" pad="BB16"/>
<connect gate="-4" pin="IO202" pad="BF14"/>
<connect gate="-4" pin="IO203" pad="F16"/>
<connect gate="-4" pin="IO211" pad="BA17"/>
<connect gate="-4" pin="IO212" pad="B14"/>
<connect gate="-4" pin="IO213" pad="G17"/>
<connect gate="-4" pin="IO221" pad="BD14"/>
<connect gate="-4" pin="IO222" pad="BE15"/>
<connect gate="-4" pin="IO223" pad="C15"/>
<connect gate="-4" pin="IO231" pad="A15"/>
<connect gate="-4" pin="IO232" pad="BG15"/>
<connect gate="-4" pin="IO233" pad="D14"/>
<connect gate="-4" pin="IO241" pad="BD16"/>
<connect gate="-4" pin="IO242" pad="D16"/>
<connect gate="-5" pin="IO251" pad="BB18"/>
<connect gate="-5" pin="IO252" pad="F18"/>
<connect gate="-5" pin="IO261" pad="BA19"/>
<connect gate="-5" pin="IO262" pad="BF16"/>
<connect gate="-5" pin="IO263" pad="B16"/>
<connect gate="-5" pin="IO271" pad="BE17"/>
<connect gate="-5" pin="IO272" pad="C17"/>
<connect gate="-5" pin="IO273" pad="G19"/>
<connect gate="-5" pin="IO281" pad="BC17"/>
<connect gate="-5" pin="IO282" pad="BG17"/>
<connect gate="-5" pin="IO283" pad="E17"/>
<connect gate="-5" pin="IO291" pad="A17"/>
<connect gate="-5" pin="IO292" pad="BD18"/>
<connect gate="-5" pin="IO293" pad="D18"/>
<connect gate="-5" pin="IO301" pad="BF18"/>
<connect gate="-5" pin="IO302" pad="B18"/>
<connect gate="-6" pin="IO311" pad="A19"/>
<connect gate="-6" pin="IO312" pad="BG19"/>
<connect gate="-6" pin="IO313" pad="F20"/>
<connect gate="-6" pin="IO321" pad="BB20"/>
<connect gate="-6" pin="IO322" pad="BF20"/>
<connect gate="-6" pin="IO323" pad="B20"/>
<connect gate="-6" pin="IO331" pad="A21"/>
<connect gate="-6" pin="IO332" pad="BA21"/>
<connect gate="-6" pin="IO333" pad="G21"/>
<connect gate="-6" pin="IO341" pad="BD20"/>
<connect gate="-6" pin="IO342" pad="BG21"/>
<connect gate="-6" pin="IO343" pad="D20"/>
<connect gate="-6" pin="IO351" pad="BF22"/>
<connect gate="-6" pin="IO352" pad="B22"/>
<connect gate="-6" pin="IO353" pad="D22"/>
<connect gate="-6" pin="IO361" pad="BB22"/>
<connect gate="-7" pin="IO362" pad="BD22"/>
<connect gate="-7" pin="IO363" pad="F22"/>
<connect gate="-7" pin="IO371" pad="BA23"/>
<connect gate="-7" pin="IO372" pad="C23"/>
<connect gate="-7" pin="IO373" pad="E23"/>
<connect gate="-7" pin="IO381" pad="A23"/>
<connect gate="-7" pin="IO382" pad="BC23"/>
<connect gate="-7" pin="IO383" pad="BE23"/>
<connect gate="-7" pin="IO391" pad="BE25"/>
<connect gate="-7" pin="IO392" pad="B26"/>
<connect gate="-7" pin="IO393" pad="E25"/>
<connect gate="-7" pin="IO401" pad="A27"/>
<connect gate="-7" pin="IO402" pad="BA25"/>
<connect gate="-7" pin="IO403" pad="BC25"/>
<connect gate="-7" pin="IO411" pad="BD26"/>
<connect gate="-7" pin="IO412" pad="F26"/>
<connect gate="-8" pin="IO421" pad="BB26"/>
<connect gate="-8" pin="IO422" pad="BF26"/>
<connect gate="-8" pin="IO423" pad="D26"/>
<connect gate="-8" pin="IO431" pad="BD28"/>
<connect gate="-8" pin="IO432" pad="B28"/>
<connect gate="-8" pin="IO433" pad="D28"/>
<connect gate="-8" pin="IO441" pad="A29"/>
<connect gate="-8" pin="IO442" pad="BA27"/>
<connect gate="-8" pin="IO443" pad="BG27"/>
<connect gate="-8" pin="IO451" pad="BF28"/>
<connect gate="-8" pin="IO452" pad="B30"/>
<connect gate="-8" pin="IO453" pad="G27"/>
<connect gate="-8" pin="IO461" pad="BB28"/>
<connect gate="-8" pin="IO462" pad="BG29"/>
<connect gate="-8" pin="IO463" pad="F28"/>
<connect gate="-8" pin="IO471" pad="A31"/>
<connect gate="-9" pin="IO481" pad="BD30"/>
<connect gate="-9" pin="IO482" pad="BF30"/>
<connect gate="-9" pin="IO483" pad="C31"/>
<connect gate="-9" pin="IO491" pad="BG31"/>
<connect gate="-9" pin="IO492" pad="B32"/>
<connect gate="-9" pin="IO493" pad="D30"/>
<connect gate="-9" pin="IO501" pad="BC31"/>
<connect gate="-9" pin="IO502" pad="BE31"/>
<connect gate="-9" pin="IO503" pad="E31"/>
<connect gate="-9" pin="IO511" pad="A33"/>
<connect gate="-9" pin="IO512" pad="BA29"/>
<connect gate="-9" pin="IO513" pad="G29"/>
<connect gate="-9" pin="IO521" pad="BB30"/>
<connect gate="-9" pin="IO522" pad="BF32"/>
<connect gate="-9" pin="IO523" pad="C33"/>
<connect gate="-9" pin="IO531" pad="D32"/>
<connect gate="-A" pin="IOA1" pad="AW9"/>
<connect gate="-A" pin="IOA10" pad="BC45"/>
<connect gate="-A" pin="IOA11" pad="BD4"/>
<connect gate="-A" pin="IOA12" pad="BF2"/>
<connect gate="-A" pin="IOA13" pad="BF46"/>
<connect gate="-A" pin="IOA2" pad="AW39"/>
<connect gate="-A" pin="IOA3" pad="AW41"/>
<connect gate="-A" pin="IOA4" pad="AY4"/>
<connect gate="-A" pin="IOA5" pad="AY6"/>
<connect gate="-A" pin="IOA6" pad="AY42"/>
<connect gate="-A" pin="IOA7" pad="AY44"/>
<connect gate="-A" pin="IOA8" pad="BB44"/>
<connect gate="-A" pin="IOA9" pad="BC3"/>
<connect gate="-B" pin="IOB1" pad="AV6"/>
<connect gate="-B" pin="IOB10" pad="BB46"/>
<connect gate="-B" pin="IOB11" pad="BD2"/>
<connect gate="-B" pin="IOB12" pad="BD46"/>
<connect gate="-B" pin="IOB2" pad="AV8"/>
<connect gate="-B" pin="IOB3" pad="AV40"/>
<connect gate="-B" pin="IOB4" pad="AV42"/>
<connect gate="-B" pin="IOB5" pad="AV44"/>
<connect gate="-B" pin="IOB6" pad="AW7"/>
<connect gate="-B" pin="IOB7" pad="BA45"/>
<connect gate="-B" pin="IOB8" pad="BB2"/>
<connect gate="-B" pin="IOB9" pad="BB4"/>
<connect gate="-C" pin="IOC1" pad="AT8"/>
<connect gate="-C" pin="IOC10" pad="AY46"/>
<connect gate="-C" pin="IOC11" pad="BA3"/>
<connect gate="-C" pin="IOC12" pad="BC1"/>
<connect gate="-C" pin="IOC13" pad="BC47"/>
<connect gate="-C" pin="IOC2" pad="AT40"/>
<connect gate="-C" pin="IOC3" pad="AT42"/>
<connect gate="-C" pin="IOC4" pad="AU5"/>
<connect gate="-C" pin="IOC5" pad="AU7"/>
<connect gate="-C" pin="IOC6" pad="AU41"/>
<connect gate="-C" pin="IOC7" pad="AU43"/>
<connect gate="-C" pin="IOC8" pad="AV4"/>
<connect gate="-C" pin="IOC9" pad="AW45"/>
<connect gate="-D" pin="IOD1" pad="AP6"/>
<connect gate="-D" pin="IOD10" pad="AW3"/>
<connect gate="-D" pin="IOD11" pad="AW47"/>
<connect gate="-D" pin="IOD12" pad="AY2"/>
<connect gate="-D" pin="IOD13" pad="BA47"/>
<connect gate="-D" pin="IOD2" pad="AP8"/>
<connect gate="-D" pin="IOD3" pad="AP40"/>
<connect gate="-D" pin="IOD4" pad="AP42"/>
<connect gate="-D" pin="IOD5" pad="AR7"/>
<connect gate="-D" pin="IOD6" pad="AR41"/>
<connect gate="-D" pin="IOD7" pad="AT4"/>
<connect gate="-D" pin="IOD8" pad="AT6"/>
<connect gate="-D" pin="IOD9" pad="AT44"/>
<connect gate="-E" pin="IOE1" pad="AM8"/>
<connect gate="-E" pin="IOE10" pad="AV46"/>
<connect gate="-E" pin="IOE11" pad="AW1"/>
<connect gate="-E" pin="IOE12" pad="BA1"/>
<connect gate="-E" pin="IOE2" pad="AM40"/>
<connect gate="-E" pin="IOE3" pad="AN7"/>
<connect gate="-E" pin="IOE4" pad="AN41"/>
<connect gate="-E" pin="IOE5" pad="AP4"/>
<connect gate="-E" pin="IOE6" pad="AP44"/>
<connect gate="-E" pin="IOE7" pad="AT46"/>
<connect gate="-E" pin="IOE8" pad="AU47"/>
<connect gate="-E" pin="IOE9" pad="AV2"/>
<connect gate="-F" pin="IOF1" pad="AK40"/>
<connect gate="-F" pin="IOF10" pad="AR47"/>
<connect gate="-F" pin="IOF11" pad="AT2"/>
<connect gate="-F" pin="IOF12" pad="AU1"/>
<connect gate="-F" pin="IOF2" pad="AL7"/>
<connect gate="-F" pin="IOF3" pad="AL41"/>
<connect gate="-F" pin="IOF4" pad="AM4"/>
<connect gate="-F" pin="IOF5" pad="AM6"/>
<connect gate="-F" pin="IOF6" pad="AM42"/>
<connect gate="-F" pin="IOF7" pad="AM44"/>
<connect gate="-F" pin="IOF8" pad="AP46"/>
<connect gate="-F" pin="IOF9" pad="AR1"/>
<connect gate="-G" pin="IOG1" pad="AK4"/>
<connect gate="-G" pin="IOG10" pad="AN3"/>
<connect gate="-G" pin="IOG11" pad="AN45"/>
<connect gate="-G" pin="IOG12" pad="AN47"/>
<connect gate="-G" pin="IOG13" pad="AP2"/>
<connect gate="-G" pin="IOG2" pad="AK6"/>
<connect gate="-G" pin="IOG3" pad="AK8"/>
<connect gate="-G" pin="IOG4" pad="AK42"/>
<connect gate="-G" pin="IOG5" pad="AK44"/>
<connect gate="-G" pin="IOG6" pad="AL5"/>
<connect gate="-G" pin="IOG7" pad="AL43"/>
<connect gate="-G" pin="IOG8" pad="AM46"/>
<connect gate="-G" pin="IOG9" pad="AN1"/>
<connect gate="-H" pin="IOH1" pad="AH6"/>
<connect gate="-H" pin="IOH10" pad="AL45"/>
<connect gate="-H" pin="IOH11" pad="AL47"/>
<connect gate="-H" pin="IOH12" pad="AM2"/>
<connect gate="-H" pin="IOH2" pad="AH8"/>
<connect gate="-H" pin="IOH3" pad="AH40"/>
<connect gate="-H" pin="IOH4" pad="AH42"/>
<connect gate="-H" pin="IOH5" pad="AJ7"/>
<connect gate="-H" pin="IOH6" pad="AJ41"/>
<connect gate="-H" pin="IOH7" pad="AK46"/>
<connect gate="-H" pin="IOH8" pad="AL1"/>
<connect gate="-H" pin="IOH9" pad="AL3"/>
<connect gate="-I" pin="IOI1" pad="AF8"/>
<connect gate="-I" pin="IOI10" pad="AH46"/>
<connect gate="-I" pin="IOI11" pad="AJ1"/>
<connect gate="-I" pin="IOI12" pad="AJ47"/>
<connect gate="-I" pin="IOI13" pad="AK2"/>
<connect gate="-I" pin="IOI2" pad="AF40"/>
<connect gate="-I" pin="IOI3" pad="AF42"/>
<connect gate="-I" pin="IOI4" pad="AG7"/>
<connect gate="-I" pin="IOI5" pad="AG41"/>
<connect gate="-I" pin="IOI6" pad="AG47"/>
<connect gate="-I" pin="IOI7" pad="AH2"/>
<connect gate="-I" pin="IOI8" pad="AH4"/>
<connect gate="-I" pin="IOI9" pad="AH44"/>
<connect gate="-J" pin="IOJ1" pad="AE3"/>
<connect gate="-J" pin="IOJ10" pad="AF6"/>
<connect gate="-J" pin="IOJ11" pad="AF44"/>
<connect gate="-J" pin="IOJ12" pad="AF46"/>
<connect gate="-J" pin="IOJ13" pad="AG1"/>
<connect gate="-J" pin="IOJ2" pad="AE5"/>
<connect gate="-J" pin="IOJ3" pad="AE7"/>
<connect gate="-J" pin="IOJ4" pad="AE41"/>
<connect gate="-J" pin="IOJ5" pad="AE43"/>
<connect gate="-J" pin="IOJ6" pad="AE45"/>
<connect gate="-J" pin="IOJ7" pad="AE47"/>
<connect gate="-J" pin="IOJ8" pad="AF2"/>
<connect gate="-J" pin="IOJ9" pad="AF4"/>
<connect gate="-K" pin="IOK1" pad="AC3"/>
<connect gate="-K" pin="IOK10" pad="AD40"/>
<connect gate="-K" pin="IOK11" pad="AD46"/>
<connect gate="-K" pin="IOK12" pad="AE1"/>
<connect gate="-K" pin="IOK2" pad="AC5"/>
<connect gate="-K" pin="IOK3" pad="AC7"/>
<connect gate="-K" pin="IOK4" pad="AC41"/>
<connect gate="-K" pin="IOK5" pad="AC43"/>
<connect gate="-K" pin="IOK6" pad="AC45"/>
<connect gate="-K" pin="IOK7" pad="AC47"/>
<connect gate="-K" pin="IOK8" pad="AD2"/>
<connect gate="-K" pin="IOK9" pad="AD8"/>
<connect gate="-L" pin="IOL1" pad="AA1"/>
<connect gate="-L" pin="IOL10" pad="AB46"/>
<connect gate="-L" pin="IOL11" pad="AC1"/>
<connect gate="-L" pin="IOL12" pad="Y46"/>
<connect gate="-L" pin="IOL2" pad="AA47"/>
<connect gate="-L" pin="IOL3" pad="AB2"/>
<connect gate="-L" pin="IOL4" pad="AB4"/>
<connect gate="-L" pin="IOL5" pad="AB6"/>
<connect gate="-L" pin="IOL6" pad="AB8"/>
<connect gate="-L" pin="IOL7" pad="AB40"/>
<connect gate="-L" pin="IOL8" pad="AB42"/>
<connect gate="-L" pin="IOL9" pad="AB44"/>
<connect gate="-M" pin="IOM1" pad="AA7"/>
<connect gate="-M" pin="IOM10" pad="Y4"/>
<connect gate="-M" pin="IOM11" pad="Y8"/>
<connect gate="-M" pin="IOM12" pad="Y40"/>
<connect gate="-M" pin="IOM13" pad="Y44"/>
<connect gate="-M" pin="IOM2" pad="AA41"/>
<connect gate="-M" pin="IOM3" pad="U45"/>
<connect gate="-M" pin="IOM4" pad="U47"/>
<connect gate="-M" pin="IOM5" pad="V2"/>
<connect gate="-M" pin="IOM6" pad="V46"/>
<connect gate="-M" pin="IOM7" pad="W1"/>
<connect gate="-M" pin="IOM8" pad="W47"/>
<connect gate="-M" pin="IOM9" pad="Y2"/>
<connect gate="-N" pin="ION1" pad="R47"/>
<connect gate="-N" pin="ION10" pad="W7"/>
<connect gate="-N" pin="ION11" pad="W41"/>
<connect gate="-N" pin="ION12" pad="Y6"/>
<connect gate="-N" pin="ION13" pad="Y42"/>
<connect gate="-N" pin="ION2" pad="T2"/>
<connect gate="-N" pin="ION3" pad="T46"/>
<connect gate="-N" pin="ION4" pad="U1"/>
<connect gate="-N" pin="ION5" pad="U3"/>
<connect gate="-N" pin="ION6" pad="V4"/>
<connect gate="-N" pin="ION7" pad="V8"/>
<connect gate="-N" pin="ION8" pad="V40"/>
<connect gate="-N" pin="ION9" pad="V44"/>
<connect gate="-O" pin="IOO1" pad="N47"/>
<connect gate="-O" pin="IOO10" pad="U41"/>
<connect gate="-O" pin="IOO11" pad="U43"/>
<connect gate="-O" pin="IOO12" pad="V6"/>
<connect gate="-O" pin="IOO13" pad="V42"/>
<connect gate="-O" pin="IOO2" pad="P2"/>
<connect gate="-O" pin="IOO3" pad="P46"/>
<connect gate="-O" pin="IOO4" pad="R1"/>
<connect gate="-O" pin="IOO5" pad="R3"/>
<connect gate="-O" pin="IOO6" pad="R45"/>
<connect gate="-O" pin="IOO7" pad="T44"/>
<connect gate="-O" pin="IOO8" pad="U5"/>
<connect gate="-O" pin="IOO9" pad="U7"/>
<connect gate="-P" pin="IOP1" pad="K46"/>
<connect gate="-P" pin="IOP10" pad="T4"/>
<connect gate="-P" pin="IOP11" pad="T6"/>
<connect gate="-P" pin="IOP12" pad="T8"/>
<connect gate="-P" pin="IOP13" pad="T40"/>
<connect gate="-P" pin="IOP14" pad="T42"/>
<connect gate="-P" pin="IOP2" pad="L1"/>
<connect gate="-P" pin="IOP3" pad="L47"/>
<connect gate="-P" pin="IOP4" pad="M2"/>
<connect gate="-P" pin="IOP5" pad="M46"/>
<connect gate="-P" pin="IOP6" pad="N1"/>
<connect gate="-P" pin="IOP7" pad="P40"/>
<connect gate="-P" pin="IOP8" pad="R7"/>
<connect gate="-P" pin="IOP9" pad="R41"/>
<connect gate="-Q" pin="IOQ1" pad="H46"/>
<connect gate="-Q" pin="IOQ10" pad="P4"/>
<connect gate="-Q" pin="IOQ11" pad="P6"/>
<connect gate="-Q" pin="IOQ12" pad="P8"/>
<connect gate="-Q" pin="IOQ13" pad="P42"/>
<connect gate="-Q" pin="IOQ14" pad="P44"/>
<connect gate="-Q" pin="IOQ2" pad="J1"/>
<connect gate="-Q" pin="IOQ3" pad="J3"/>
<connect gate="-Q" pin="IOQ4" pad="J45"/>
<connect gate="-Q" pin="IOQ5" pad="J47"/>
<connect gate="-Q" pin="IOQ6" pad="K2"/>
<connect gate="-Q" pin="IOQ7" pad="M44"/>
<connect gate="-Q" pin="IOQ8" pad="N7"/>
<connect gate="-Q" pin="IOQ9" pad="N41"/>
<connect gate="-R" pin="IOR1" pad="G1"/>
<connect gate="-R" pin="IOR10" pad="M8"/>
<connect gate="-R" pin="IOR11" pad="M40"/>
<connect gate="-R" pin="IOR12" pad="M42"/>
<connect gate="-R" pin="IOR2" pad="G47"/>
<connect gate="-R" pin="IOR3" pad="H2"/>
<connect gate="-R" pin="IOR4" pad="H44"/>
<connect gate="-R" pin="IOR5" pad="L5"/>
<connect gate="-R" pin="IOR6" pad="L41"/>
<connect gate="-R" pin="IOR7" pad="L43"/>
<connect gate="-R" pin="IOR8" pad="M4"/>
<connect gate="-R" pin="IOR9" pad="M6"/>
<connect gate="-S" pin="IOS1" pad="F2"/>
<connect gate="-S" pin="IOS10" pad="K40"/>
<connect gate="-S" pin="IOS11" pad="K42"/>
<connect gate="-S" pin="IOS12" pad="K44"/>
<connect gate="-S" pin="IOS13" pad="L7"/>
<connect gate="-S" pin="IOS2" pad="F44"/>
<connect gate="-S" pin="IOS3" pad="F46"/>
<connect gate="-S" pin="IOS4" pad="G3"/>
<connect gate="-S" pin="IOS5" pad="G45"/>
<connect gate="-S" pin="IOS6" pad="H4"/>
<connect gate="-S" pin="IOS7" pad="K4"/>
<connect gate="-S" pin="IOS8" pad="K6"/>
<connect gate="-S" pin="IOS9" pad="K8"/>
<connect gate="-T" pin="IOT1" pad="D2"/>
<connect gate="-T" pin="IOT10" pad="H8"/>
<connect gate="-T" pin="IOT11" pad="H42"/>
<connect gate="-T" pin="IOT12" pad="J7"/>
<connect gate="-T" pin="IOT13" pad="J39"/>
<connect gate="-T" pin="IOT14" pad="J41"/>
<connect gate="-T" pin="IOT2" pad="D44"/>
<connect gate="-T" pin="IOT3" pad="D46"/>
<connect gate="-T" pin="IOT4" pad="E1"/>
<connect gate="-T" pin="IOT5" pad="E3"/>
<connect gate="-T" pin="IOT6" pad="E45"/>
<connect gate="-T" pin="IOT7" pad="E47"/>
<connect gate="-T" pin="IOT8" pad="F4"/>
<connect gate="-T" pin="IOT9" pad="H6"/>
<connect gate="GI1" pin="GND" pad="AA3"/>
<connect gate="GI10" pin="GND" pad="BE13"/>
<connect gate="GI11" pin="GND" pad="BE21"/>
<connect gate="GI12" pin="GND" pad="BE27"/>
<connect gate="GI13" pin="GND" pad="BE35"/>
<connect gate="GI14" pin="GND" pad="BE45"/>
<connect gate="GI15" pin="GND" pad="BG1"/>
<connect gate="GI16" pin="GND" pad="BG47"/>
<connect gate="GI17" pin="GND" pad="B2"/>
<connect gate="GI18" pin="GND" pad="C13"/>
<connect gate="GI19" pin="GND" pad="C21"/>
<connect gate="GI2" pin="GND" pad="AA45"/>
<connect gate="GI20" pin="GND" pad="C27"/>
<connect gate="GI21" pin="GND" pad="C35"/>
<connect gate="GI22" pin="GND" pad="C45"/>
<connect gate="GI23" pin="GND" pad="D4"/>
<connect gate="GI24" pin="GND" pad="G23"/>
<connect gate="GI25" pin="GND" pad="N3"/>
<connect gate="GI26" pin="GND" pad="N45"/>
<connect gate="GI3" pin="GND" pad="AG3"/>
<connect gate="GI4" pin="GND" pad="AG45"/>
<connect gate="GI5" pin="GND" pad="AR3"/>
<connect gate="GI6" pin="GND" pad="AR45"/>
<connect gate="GI7" pin="GND" pad="A47"/>
<connect gate="GI8" pin="GND" pad="BD44"/>
<connect gate="GI9" pin="GND" pad="BE3"/>
<connect gate="GO1" pin="GNDIO" pad="AD6"/>
<connect gate="GO10" pin="GNDIO" pad="BA43"/>
<connect gate="GO11" pin="GNDIO" pad="BB24"/>
<connect gate="GO12" pin="GNDIO" pad="BC7"/>
<connect gate="GO13" pin="GNDIO" pad="BC13"/>
<connect gate="GO14" pin="GNDIO" pad="BC19"/>
<connect gate="GO15" pin="GNDIO" pad="BC29"/>
<connect gate="GO16" pin="GNDIO" pad="BC35"/>
<connect gate="GO17" pin="GNDIO" pad="BC41"/>
<connect gate="GO18" pin="GNDIO" pad="E7"/>
<connect gate="GO19" pin="GNDIO" pad="E13"/>
<connect gate="GO2" pin="GNDIO" pad="AD42"/>
<connect gate="GO20" pin="GNDIO" pad="E19"/>
<connect gate="GO21" pin="GNDIO" pad="E29"/>
<connect gate="GO22" pin="GNDIO" pad="E35"/>
<connect gate="GO23" pin="GNDIO" pad="E41"/>
<connect gate="GO24" pin="GNDIO" pad="F24"/>
<connect gate="GO25" pin="GNDIO" pad="G5"/>
<connect gate="GO26" pin="GNDIO" pad="G43"/>
<connect gate="GO27" pin="GNDIO" pad="H40"/>
<connect gate="GO28" pin="GNDIO" pad="N5"/>
<connect gate="GO29" pin="GNDIO" pad="N43"/>
<connect gate="GO3" pin="GNDIO" pad="AJ5"/>
<connect gate="GO30" pin="GNDIO" pad="W5"/>
<connect gate="GO31" pin="GNDIO" pad="W43"/>
<connect gate="GO4" pin="GNDIO" pad="AJ43"/>
<connect gate="GO5" pin="GNDIO" pad="AR5"/>
<connect gate="GO6" pin="GNDIO" pad="AR43"/>
<connect gate="GO7" pin="GNDIO" pad="AY8"/>
<connect gate="GO8" pin="GNDIO" pad="AY40"/>
<connect gate="GO9" pin="GNDIO" pad="BA5"/>
<connect gate="V1" pin="VCC" pad="AJ3"/>
<connect gate="V10" pin="VCC" pad="BE29"/>
<connect gate="V11" pin="VCC" pad="BE37"/>
<connect gate="V12" pin="VCC" pad="BE47"/>
<connect gate="V13" pin="VCC" pad="BG3"/>
<connect gate="V14" pin="VCC" pad="BG45"/>
<connect gate="V15" pin="VCC" pad="C1"/>
<connect gate="V16" pin="VCC" pad="C11"/>
<connect gate="V17" pin="VCC" pad="C19"/>
<connect gate="V18" pin="VCC" pad="C29"/>
<connect gate="V19" pin="VCC" pad="C37"/>
<connect gate="V2" pin="VCC" pad="AJ45"/>
<connect gate="V20" pin="VCC" pad="C47"/>
<connect gate="V21" pin="VCC" pad="E5"/>
<connect gate="V22" pin="VCC" pad="G25"/>
<connect gate="V23" pin="VCC" pad="L3"/>
<connect gate="V24" pin="VCC" pad="L45"/>
<connect gate="V25" pin="VCC" pad="W3"/>
<connect gate="V26" pin="VCC" pad="W45"/>
<connect gate="V3" pin="VCC" pad="AU3"/>
<connect gate="V4" pin="VCC" pad="AU45"/>
<connect gate="V5" pin="VCC" pad="A3"/>
<connect gate="V6" pin="VCC" pad="A45"/>
<connect gate="V7" pin="VCC" pad="BE1"/>
<connect gate="V8" pin="VCC" pad="BE11"/>
<connect gate="V9" pin="VCC" pad="BE19"/>
<connect gate="VO1" pin="VCCIO" pad="AA5"/>
<connect gate="VO10" pin="VCCIO" pad="AW43"/>
<connect gate="VO11" pin="VCCIO" pad="BA7"/>
<connect gate="VO12" pin="VCCIO" pad="BA41"/>
<connect gate="VO13" pin="VCCIO" pad="BC9"/>
<connect gate="VO14" pin="VCCIO" pad="BC15"/>
<connect gate="VO15" pin="VCCIO" pad="BC21"/>
<connect gate="VO16" pin="VCCIO" pad="BC27"/>
<connect gate="VO17" pin="VCCIO" pad="BC33"/>
<connect gate="VO18" pin="VCCIO" pad="BC39"/>
<connect gate="VO19" pin="VCCIO" pad="BD24"/>
<connect gate="VO2" pin="VCCIO" pad="AA43"/>
<connect gate="VO20" pin="VCCIO" pad="D24"/>
<connect gate="VO21" pin="VCCIO" pad="E9"/>
<connect gate="VO22" pin="VCCIO" pad="E15"/>
<connect gate="VO23" pin="VCCIO" pad="E21"/>
<connect gate="VO24" pin="VCCIO" pad="E27"/>
<connect gate="VO25" pin="VCCIO" pad="E33"/>
<connect gate="VO26" pin="VCCIO" pad="E39"/>
<connect gate="VO27" pin="VCCIO" pad="G7"/>
<connect gate="VO28" pin="VCCIO" pad="G41"/>
<connect gate="VO29" pin="VCCIO" pad="J5"/>
<connect gate="VO3" pin="VCCIO" pad="AD4"/>
<connect gate="VO30" pin="VCCIO" pad="J43"/>
<connect gate="VO31" pin="VCCIO" pad="R5"/>
<connect gate="VO32" pin="VCCIO" pad="R43"/>
<connect gate="VO4" pin="VCCIO" pad="AD44"/>
<connect gate="VO5" pin="VCCIO" pad="AG5"/>
<connect gate="VO6" pin="VCCIO" pad="AG43"/>
<connect gate="VO7" pin="VCCIO" pad="AN5"/>
<connect gate="VO8" pin="VCCIO" pad="AN43"/>
<connect gate="VO9" pin="VCCIO" pad="AW5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K250-BGA600" prefix="IC">
<description>&lt;b&gt;EPF10K250&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="K240C"/>
<gate name="-A" symbol="A13-600"/>
<gate name="-B" symbol="B12-600"/>
<gate name="-C" symbol="C13-600"/>
<gate name="-D" symbol="D13-600"/>
<gate name="-E" symbol="E12-600"/>
<gate name="-F" symbol="F12-600"/>
<gate name="-G" symbol="G13-600"/>
<gate name="-H" symbol="H12-600"/>
<gate name="-I" symbol="I13-600"/>
<gate name="-J" symbol="J13-600"/>
<gate name="-K" symbol="K12-600"/>
<gate name="-L" symbol="L12-600"/>
<gate name="-M" symbol="M13-600"/>
<gate name="-N" symbol="N13-600"/>
<gate name="-O" symbol="O13-600"/>
<gate name="-P" symbol="P14-600"/>
<gate name="-Q" symbol="Q14-600"/>
<gate name="-R" symbol="R12-600"/>
<gate name="-S" symbol="S13-600"/>
<gate name="-T" symbol="T14-600"/>
<gate name="-1" symbol="62-600"/>
<gate name="-2" symbol="122-600"/>
<gate name="-3" symbol="182-600"/>
<gate name="-4" symbol="242-600"/>
<gate name="-5" symbol="302-600"/>
<gate name="-6" symbol="361-600"/>
<gate name="-7" symbol="412-600"/>
<gate name="-8" symbol="471-600"/>
<gate name="-9" symbol="531-600"/>
<gate name="-10" symbol="583-600"/>
<gate name="-11" symbol="642-600"/>
<gate name="-12" symbol="702-600"/>
<gate name="-13" symbol="762-600"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="G50" symbol="GND"/>
<gate name="G51" symbol="GND"/>
<gate name="G52" symbol="GND"/>
<gate name="G53" symbol="GND"/>
<gate name="G54" symbol="GND"/>
<gate name="G55" symbol="GND"/>
<gate name="G56" symbol="GND"/>
<gate name="G57" symbol="GND"/>
<gate name="G58" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="V24" symbol="VCCINT"/>
<gate name="V25" symbol="VCCINT"/>
<gate name="V26" symbol="VCCINT"/>
<gate name="V27" symbol="VCCINT"/>
<gate name="V28" symbol="VCCINT"/>
<gate name="V29" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="BGA600">
<connects>
<connect gate="-1" pin="IO11" pad="AR6"/>
<connect gate="-1" pin="IO12" pad="A6"/>
<connect gate="-1" pin="IO21" pad="AM7"/>
<connect gate="-1" pin="IO22" pad="AL7"/>
<connect gate="-1" pin="IO23" pad="E7"/>
<connect gate="-1" pin="IO31" pad="AN7"/>
<connect gate="-1" pin="IO32" pad="C7"/>
<connect gate="-1" pin="IO33" pad="D7"/>
<connect gate="-1" pin="IO41" pad="AP7"/>
<connect gate="-1" pin="IO42" pad="AR7"/>
<connect gate="-1" pin="IO43" pad="B7"/>
<connect gate="-1" pin="IO51" pad="AL8"/>
<connect gate="-1" pin="IO52" pad="A7"/>
<connect gate="-1" pin="IO53" pad="E8"/>
<connect gate="-1" pin="IO61" pad="AM8"/>
<connect gate="-1" pin="IO62" pad="D8"/>
<connect gate="-10" pin="IO532" pad="B23"/>
<connect gate="-10" pin="IO541" pad="AP23"/>
<connect gate="-10" pin="IO542" pad="AN23"/>
<connect gate="-10" pin="IO543" pad="E23"/>
<connect gate="-10" pin="IO551" pad="B24"/>
<connect gate="-10" pin="IO552" pad="AM23"/>
<connect gate="-10" pin="IO553" pad="A24"/>
<connect gate="-10" pin="IO561" pad="AR24"/>
<connect gate="-10" pin="IO562" pad="AL23"/>
<connect gate="-10" pin="IO563" pad="C24"/>
<connect gate="-10" pin="IO571" pad="AN24"/>
<connect gate="-10" pin="IO572" pad="A25"/>
<connect gate="-10" pin="IO573" pad="B25"/>
<connect gate="-10" pin="IO581" pad="E24"/>
<connect gate="-10" pin="IO582" pad="AM24"/>
<connect gate="-10" pin="IO583" pad="AR25"/>
<connect gate="-11" pin="IO591" pad="C25"/>
<connect gate="-11" pin="IO592" pad="AP25"/>
<connect gate="-11" pin="IO601" pad="AL24"/>
<connect gate="-11" pin="IO602" pad="AN25"/>
<connect gate="-11" pin="IO603" pad="D25"/>
<connect gate="-11" pin="IO611" pad="AM25"/>
<connect gate="-11" pin="IO612" pad="E25"/>
<connect gate="-11" pin="IO613" pad="A26"/>
<connect gate="-11" pin="IO621" pad="B26"/>
<connect gate="-11" pin="IO622" pad="AR26"/>
<connect gate="-11" pin="IO623" pad="AL25"/>
<connect gate="-11" pin="IO631" pad="AP26"/>
<connect gate="-11" pin="IO632" pad="D26"/>
<connect gate="-11" pin="IO633" pad="C26"/>
<connect gate="-11" pin="IO641" pad="AN26"/>
<connect gate="-11" pin="IO642" pad="E26"/>
<connect gate="-12" pin="IO651" pad="AL26"/>
<connect gate="-12" pin="IO652" pad="B27"/>
<connect gate="-12" pin="IO661" pad="AP27"/>
<connect gate="-12" pin="IO662" pad="AR27"/>
<connect gate="-12" pin="IO663" pad="C27"/>
<connect gate="-12" pin="IO671" pad="AN27"/>
<connect gate="-12" pin="IO672" pad="E27"/>
<connect gate="-12" pin="IO673" pad="D27"/>
<connect gate="-12" pin="IO681" pad="AM27"/>
<connect gate="-12" pin="IO682" pad="AL27"/>
<connect gate="-12" pin="IO683" pad="A28"/>
<connect gate="-12" pin="IO691" pad="B28"/>
<connect gate="-12" pin="IO692" pad="AR28"/>
<connect gate="-12" pin="IO693" pad="C28"/>
<connect gate="-12" pin="IO701" pad="AP28"/>
<connect gate="-12" pin="IO702" pad="D28"/>
<connect gate="-13" pin="IO711" pad="AN28"/>
<connect gate="-13" pin="IO712" pad="E28"/>
<connect gate="-13" pin="IO721" pad="AM28"/>
<connect gate="-13" pin="IO722" pad="AL28"/>
<connect gate="-13" pin="IO723" pad="A29"/>
<connect gate="-13" pin="IO731" pad="AR29"/>
<connect gate="-13" pin="IO732" pad="B29"/>
<connect gate="-13" pin="IO733" pad="C29"/>
<connect gate="-13" pin="IO741" pad="AN29"/>
<connect gate="-13" pin="IO742" pad="AP29"/>
<connect gate="-13" pin="IO743" pad="D29"/>
<connect gate="-13" pin="IO751" pad="AM29"/>
<connect gate="-13" pin="IO752" pad="A30"/>
<connect gate="-13" pin="IO753" pad="E29"/>
<connect gate="-13" pin="IO761" pad="AL29"/>
<connect gate="-13" pin="IO762" pad="B30"/>
<connect gate="-2" pin="IO101" pad="AP9"/>
<connect gate="-2" pin="IO102" pad="AN9"/>
<connect gate="-2" pin="IO103" pad="C9"/>
<connect gate="-2" pin="IO111" pad="A9"/>
<connect gate="-2" pin="IO112" pad="AR9"/>
<connect gate="-2" pin="IO113" pad="B9"/>
<connect gate="-2" pin="IO121" pad="AL10"/>
<connect gate="-2" pin="IO122" pad="E10"/>
<connect gate="-2" pin="IO71" pad="B8"/>
<connect gate="-2" pin="IO72" pad="AP8"/>
<connect gate="-2" pin="IO81" pad="AR8"/>
<connect gate="-2" pin="IO82" pad="AL9"/>
<connect gate="-2" pin="IO83" pad="A8"/>
<connect gate="-2" pin="IO91" pad="AM9"/>
<connect gate="-2" pin="IO92" pad="E9"/>
<connect gate="-2" pin="IO93" pad="D9"/>
<connect gate="-3" pin="IO131" pad="AM10"/>
<connect gate="-3" pin="IO132" pad="D10"/>
<connect gate="-3" pin="IO141" pad="AP10"/>
<connect gate="-3" pin="IO142" pad="AN10"/>
<connect gate="-3" pin="IO143" pad="C10"/>
<connect gate="-3" pin="IO151" pad="A10"/>
<connect gate="-3" pin="IO152" pad="AR10"/>
<connect gate="-3" pin="IO153" pad="B10"/>
<connect gate="-3" pin="IO161" pad="AL11"/>
<connect gate="-3" pin="IO162" pad="AM11"/>
<connect gate="-3" pin="IO163" pad="E11"/>
<connect gate="-3" pin="IO171" pad="D11"/>
<connect gate="-3" pin="IO172" pad="AN11"/>
<connect gate="-3" pin="IO173" pad="C11"/>
<connect gate="-3" pin="IO181" pad="AP11"/>
<connect gate="-3" pin="IO182" pad="B11"/>
<connect gate="-4" pin="IO191" pad="D12"/>
<connect gate="-4" pin="IO192" pad="AM12"/>
<connect gate="-4" pin="IO201" pad="AN12"/>
<connect gate="-4" pin="IO202" pad="AP12"/>
<connect gate="-4" pin="IO203" pad="C12"/>
<connect gate="-4" pin="IO211" pad="AR12"/>
<connect gate="-4" pin="IO212" pad="B12"/>
<connect gate="-4" pin="IO213" pad="A12"/>
<connect gate="-4" pin="IO221" pad="AM13"/>
<connect gate="-4" pin="IO222" pad="AL13"/>
<connect gate="-4" pin="IO223" pad="E13"/>
<connect gate="-4" pin="IO231" pad="C13"/>
<connect gate="-4" pin="IO232" pad="AN13"/>
<connect gate="-4" pin="IO233" pad="D13"/>
<connect gate="-4" pin="IO241" pad="AP13"/>
<connect gate="-4" pin="IO242" pad="B13"/>
<connect gate="-5" pin="IO251" pad="AR13"/>
<connect gate="-5" pin="IO252" pad="A13"/>
<connect gate="-5" pin="IO261" pad="AM14"/>
<connect gate="-5" pin="IO262" pad="AL14"/>
<connect gate="-5" pin="IO263" pad="E14"/>
<connect gate="-5" pin="IO271" pad="AN14"/>
<connect gate="-5" pin="IO272" pad="C14"/>
<connect gate="-5" pin="IO273" pad="D14"/>
<connect gate="-5" pin="IO281" pad="AP14"/>
<connect gate="-5" pin="IO282" pad="AR14"/>
<connect gate="-5" pin="IO283" pad="B14"/>
<connect gate="-5" pin="IO291" pad="A14"/>
<connect gate="-5" pin="IO292" pad="AL15"/>
<connect gate="-5" pin="IO293" pad="E15"/>
<connect gate="-5" pin="IO301" pad="AM15"/>
<connect gate="-5" pin="IO302" pad="D15"/>
<connect gate="-6" pin="IO311" pad="B15"/>
<connect gate="-6" pin="IO312" pad="AP15"/>
<connect gate="-6" pin="IO313" pad="A15"/>
<connect gate="-6" pin="IO321" pad="AR15"/>
<connect gate="-6" pin="IO322" pad="AL16"/>
<connect gate="-6" pin="IO323" pad="E16"/>
<connect gate="-6" pin="IO331" pad="C16"/>
<connect gate="-6" pin="IO332" pad="AM16"/>
<connect gate="-6" pin="IO333" pad="D16"/>
<connect gate="-6" pin="IO341" pad="AP16"/>
<connect gate="-6" pin="IO342" pad="AN16"/>
<connect gate="-6" pin="IO343" pad="B16"/>
<connect gate="-6" pin="IO351" pad="AR16"/>
<connect gate="-6" pin="IO352" pad="A16"/>
<connect gate="-6" pin="IO353" pad="E17"/>
<connect gate="-6" pin="IO361" pad="AL17"/>
<connect gate="-7" pin="IO362" pad="AM17"/>
<connect gate="-7" pin="IO363" pad="D17"/>
<connect gate="-7" pin="IO371" pad="AN17"/>
<connect gate="-7" pin="IO372" pad="C17"/>
<connect gate="-7" pin="IO373" pad="B17"/>
<connect gate="-7" pin="IO381" pad="A17"/>
<connect gate="-7" pin="IO382" pad="AP17"/>
<connect gate="-7" pin="IO383" pad="AR17"/>
<connect gate="-7" pin="IO391" pad="AP18"/>
<connect gate="-7" pin="IO392" pad="B19"/>
<connect gate="-7" pin="IO393" pad="C19"/>
<connect gate="-7" pin="IO401" pad="D19"/>
<connect gate="-7" pin="IO402" pad="AP19"/>
<connect gate="-7" pin="IO403" pad="AR19"/>
<connect gate="-7" pin="IO411" pad="AN19"/>
<connect gate="-7" pin="IO412" pad="E19"/>
<connect gate="-8" pin="IO421" pad="AL19"/>
<connect gate="-8" pin="IO422" pad="AR20"/>
<connect gate="-8" pin="IO423" pad="B20"/>
<connect gate="-8" pin="IO431" pad="AP20"/>
<connect gate="-8" pin="IO432" pad="C20"/>
<connect gate="-8" pin="IO433" pad="D20"/>
<connect gate="-8" pin="IO441" pad="E20"/>
<connect gate="-8" pin="IO442" pad="AM20"/>
<connect gate="-8" pin="IO443" pad="AN20"/>
<connect gate="-8" pin="IO451" pad="AL20"/>
<connect gate="-8" pin="IO452" pad="B21"/>
<connect gate="-8" pin="IO453" pad="A21"/>
<connect gate="-8" pin="IO461" pad="AR21"/>
<connect gate="-8" pin="IO462" pad="AP21"/>
<connect gate="-8" pin="IO463" pad="C21"/>
<connect gate="-8" pin="IO471" pad="D21"/>
<connect gate="-9" pin="IO481" pad="AM21"/>
<connect gate="-9" pin="IO482" pad="AN21"/>
<connect gate="-9" pin="IO483" pad="E21"/>
<connect gate="-9" pin="IO491" pad="AL21"/>
<connect gate="-9" pin="IO492" pad="B22"/>
<connect gate="-9" pin="IO493" pad="A22"/>
<connect gate="-9" pin="IO501" pad="AR22"/>
<connect gate="-9" pin="IO502" pad="AP22"/>
<connect gate="-9" pin="IO503" pad="C22"/>
<connect gate="-9" pin="IO511" pad="D22"/>
<connect gate="-9" pin="IO512" pad="AN22"/>
<connect gate="-9" pin="IO513" pad="E22"/>
<connect gate="-9" pin="IO521" pad="AL22"/>
<connect gate="-9" pin="IO522" pad="AM22"/>
<connect gate="-9" pin="IO523" pad="A23"/>
<connect gate="-9" pin="IO531" pad="D23"/>
<connect gate="-A" pin="IOA1" pad="AK5"/>
<connect gate="-A" pin="IOA10" pad="AM35"/>
<connect gate="-A" pin="IOA11" pad="AL4"/>
<connect gate="-A" pin="IOA12" pad="AM2"/>
<connect gate="-A" pin="IOA13" pad="AM33"/>
<connect gate="-A" pin="IOA2" pad="AL32"/>
<connect gate="-A" pin="IOA3" pad="AL33"/>
<connect gate="-A" pin="IOA4" pad="AM1"/>
<connect gate="-A" pin="IOA5" pad="AM3"/>
<connect gate="-A" pin="IOA6" pad="AM34"/>
<connect gate="-A" pin="IOA7" pad="AJ31"/>
<connect gate="-A" pin="IOA8" pad="AK32"/>
<connect gate="-A" pin="IOA9" pad="AJ5"/>
<connect gate="-B" pin="IOB1" pad="AJ4"/>
<connect gate="-B" pin="IOB10" pad="AK33"/>
<connect gate="-B" pin="IOB11" pad="AK3"/>
<connect gate="-B" pin="IOB12" pad="AL34"/>
<connect gate="-B" pin="IOB2" pad="AL1"/>
<connect gate="-B" pin="IOB3" pad="AL35"/>
<connect gate="-B" pin="IOB4" pad="AJ32"/>
<connect gate="-B" pin="IOB5" pad="AK34"/>
<connect gate="-B" pin="IOB6" pad="AL2"/>
<connect gate="-B" pin="IOB7" pad="AH31"/>
<connect gate="-B" pin="IOB8" pad="AH5"/>
<connect gate="-B" pin="IOB9" pad="AK4"/>
<connect gate="-C" pin="IOC1" pad="AJ2"/>
<connect gate="-C" pin="IOC10" pad="AG31"/>
<connect gate="-C" pin="IOC11" pad="AK1"/>
<connect gate="-C" pin="IOC12" pad="AH4"/>
<connect gate="-C" pin="IOC13" pad="AJ35"/>
<connect gate="-C" pin="IOC2" pad="AJ33"/>
<connect gate="-C" pin="IOC3" pad="AH33"/>
<connect gate="-C" pin="IOC4" pad="AJ1"/>
<connect gate="-C" pin="IOC5" pad="AJ3"/>
<connect gate="-C" pin="IOC6" pad="AJ34"/>
<connect gate="-C" pin="IOC7" pad="AH32"/>
<connect gate="-C" pin="IOC8" pad="AK2"/>
<connect gate="-C" pin="IOC9" pad="AH34"/>
<connect gate="-D" pin="IOD1" pad="AF5"/>
<connect gate="-D" pin="IOD10" pad="AG4"/>
<connect gate="-D" pin="IOD11" pad="AG35"/>
<connect gate="-D" pin="IOD12" pad="AH2"/>
<connect gate="-D" pin="IOD13" pad="AG34"/>
<connect gate="-D" pin="IOD2" pad="AG2"/>
<connect gate="-D" pin="IOD3" pad="AG32"/>
<connect gate="-D" pin="IOD4" pad="AF31"/>
<connect gate="-D" pin="IOD5" pad="AG3"/>
<connect gate="-D" pin="IOD6" pad="AG33"/>
<connect gate="-D" pin="IOD7" pad="AH1"/>
<connect gate="-D" pin="IOD8" pad="AH3"/>
<connect gate="-D" pin="IOD9" pad="AH35"/>
<connect gate="-E" pin="IOE1" pad="AE5"/>
<connect gate="-E" pin="IOE10" pad="AF34"/>
<connect gate="-E" pin="IOE11" pad="AF3"/>
<connect gate="-E" pin="IOE12" pad="AG1"/>
<connect gate="-E" pin="IOE2" pad="AE32"/>
<connect gate="-E" pin="IOE3" pad="AF2"/>
<connect gate="-E" pin="IOE4" pad="AF35"/>
<connect gate="-E" pin="IOE5" pad="AF4"/>
<connect gate="-E" pin="IOE6" pad="AF33"/>
<connect gate="-E" pin="IOE7" pad="AE33"/>
<connect gate="-E" pin="IOE8" pad="AE31"/>
<connect gate="-E" pin="IOE9" pad="AF1"/>
<connect gate="-F" pin="IOF1" pad="AD34"/>
<connect gate="-F" pin="IOF10" pad="AE35"/>
<connect gate="-F" pin="IOF11" pad="AE1"/>
<connect gate="-F" pin="IOF12" pad="AE3"/>
<connect gate="-F" pin="IOF2" pad="AD3"/>
<connect gate="-F" pin="IOF3" pad="AD33"/>
<connect gate="-F" pin="IOF4" pad="AD5"/>
<connect gate="-F" pin="IOF5" pad="AE2"/>
<connect gate="-F" pin="IOF6" pad="AE34"/>
<connect gate="-F" pin="IOF7" pad="AD31"/>
<connect gate="-F" pin="IOF8" pad="AD32"/>
<connect gate="-F" pin="IOF9" pad="AD4"/>
<connect gate="-G" pin="IOG1" pad="AC2"/>
<connect gate="-G" pin="IOG10" pad="AC3"/>
<connect gate="-G" pin="IOG11" pad="AC32"/>
<connect gate="-G" pin="IOG12" pad="AC34"/>
<connect gate="-G" pin="IOG13" pad="AD2"/>
<connect gate="-G" pin="IOG2" pad="AC4"/>
<connect gate="-G" pin="IOG3" pad="AC5"/>
<connect gate="-G" pin="IOG4" pad="AC33"/>
<connect gate="-G" pin="IOG5" pad="AC35"/>
<connect gate="-G" pin="IOG6" pad="AD1"/>
<connect gate="-G" pin="IOG7" pad="AC31"/>
<connect gate="-G" pin="IOG8" pad="AB31"/>
<connect gate="-G" pin="IOG9" pad="AC1"/>
<connect gate="-H" pin="IOH1" pad="AA5"/>
<connect gate="-H" pin="IOH10" pad="AB33"/>
<connect gate="-H" pin="IOH11" pad="AB35"/>
<connect gate="-H" pin="IOH12" pad="AB3"/>
<connect gate="-H" pin="IOH2" pad="AB2"/>
<connect gate="-H" pin="IOH3" pad="AB34"/>
<connect gate="-H" pin="IOH4" pad="AA31"/>
<connect gate="-H" pin="IOH5" pad="AB4"/>
<connect gate="-H" pin="IOH6" pad="AB32"/>
<connect gate="-H" pin="IOH7" pad="AA32"/>
<connect gate="-H" pin="IOH8" pad="AA4"/>
<connect gate="-H" pin="IOH9" pad="AB1"/>
<connect gate="-I" pin="IOI1" pad="Y4"/>
<connect gate="-I" pin="IOI10" pad="Y32"/>
<connect gate="-I" pin="IOI11" pad="Y5"/>
<connect gate="-I" pin="IOI12" pad="AA35"/>
<connect gate="-I" pin="IOI13" pad="AA2"/>
<connect gate="-I" pin="IOI2" pad="Y33"/>
<connect gate="-I" pin="IOI3" pad="Y35"/>
<connect gate="-I" pin="IOI4" pad="AA3"/>
<connect gate="-I" pin="IOI5" pad="AA34"/>
<connect gate="-I" pin="IOI6" pad="Y34"/>
<connect gate="-I" pin="IOI7" pad="Y3"/>
<connect gate="-I" pin="IOI8" pad="AA1"/>
<connect gate="-I" pin="IOI9" pad="Y31"/>
<connect gate="-J" pin="IOJ1" pad="W1"/>
<connect gate="-J" pin="IOJ10" pad="Y1"/>
<connect gate="-J" pin="IOJ11" pad="W32"/>
<connect gate="-J" pin="IOJ12" pad="W31"/>
<connect gate="-J" pin="IOJ13" pad="W5"/>
<connect gate="-J" pin="IOJ2" pad="V5"/>
<connect gate="-J" pin="IOJ3" pad="W2"/>
<connect gate="-J" pin="IOJ4" pad="W34"/>
<connect gate="-J" pin="IOJ5" pad="V31"/>
<connect gate="-J" pin="IOJ6" pad="W33"/>
<connect gate="-J" pin="IOJ7" pad="W35"/>
<connect gate="-J" pin="IOJ8" pad="W3"/>
<connect gate="-J" pin="IOJ9" pad="W4"/>
<connect gate="-K" pin="IOK1" pad="U5"/>
<connect gate="-K" pin="IOK10" pad="V34"/>
<connect gate="-K" pin="IOK11" pad="V33"/>
<connect gate="-K" pin="IOK12" pad="V4"/>
<connect gate="-K" pin="IOK2" pad="V1"/>
<connect gate="-K" pin="IOK3" pad="U4"/>
<connect gate="-K" pin="IOK4" pad="U33"/>
<connect gate="-K" pin="IOK5" pad="U31"/>
<connect gate="-K" pin="IOK6" pad="V35"/>
<connect gate="-K" pin="IOK7" pad="U32"/>
<connect gate="-K" pin="IOK8" pad="V2"/>
<connect gate="-K" pin="IOK9" pad="V3"/>
<connect gate="-L" pin="IOL1" pad="T3"/>
<connect gate="-L" pin="IOL10" pad="U34"/>
<connect gate="-L" pin="IOL11" pad="U2"/>
<connect gate="-L" pin="IOL12" pad="T33"/>
<connect gate="-L" pin="IOL2" pad="T31"/>
<connect gate="-L" pin="IOL3" pad="T5"/>
<connect gate="-L" pin="IOL4" pad="U1"/>
<connect gate="-L" pin="IOL5" pad="T2"/>
<connect gate="-L" pin="IOL6" pad="T4"/>
<connect gate="-L" pin="IOL7" pad="T32"/>
<connect gate="-L" pin="IOL8" pad="T34"/>
<connect gate="-L" pin="IOL9" pad="U35"/>
<connect gate="-M" pin="IOM1" pad="R5"/>
<connect gate="-M" pin="IOM10" pad="R3"/>
<connect gate="-M" pin="IOM11" pad="R1"/>
<connect gate="-M" pin="IOM12" pad="P31"/>
<connect gate="-M" pin="IOM13" pad="R34"/>
<connect gate="-M" pin="IOM2" pad="R32"/>
<connect gate="-M" pin="IOM3" pad="P32"/>
<connect gate="-M" pin="IOM4" pad="R35"/>
<connect gate="-M" pin="IOM5" pad="R2"/>
<connect gate="-M" pin="IOM6" pad="R33"/>
<connect gate="-M" pin="IOM7" pad="R4"/>
<connect gate="-M" pin="IOM8" pad="R31"/>
<connect gate="-M" pin="IOM9" pad="T1"/>
<connect gate="-N" pin="ION1" pad="N33"/>
<connect gate="-N" pin="ION10" pad="P1"/>
<connect gate="-N" pin="ION11" pad="P35"/>
<connect gate="-N" pin="ION12" pad="P3"/>
<connect gate="-N" pin="ION13" pad="P33"/>
<connect gate="-N" pin="ION2" pad="N5"/>
<connect gate="-N" pin="ION3" pad="P34"/>
<connect gate="-N" pin="ION4" pad="P4"/>
<connect gate="-N" pin="ION5" pad="P2"/>
<connect gate="-N" pin="ION6" pad="N4"/>
<connect gate="-N" pin="ION7" pad="N3"/>
<connect gate="-N" pin="ION8" pad="N31"/>
<connect gate="-N" pin="ION9" pad="N32"/>
<connect gate="-O" pin="IOO1" pad="M34"/>
<connect gate="-O" pin="IOO10" pad="M33"/>
<connect gate="-O" pin="IOO11" pad="M31"/>
<connect gate="-O" pin="IOO12" pad="N2"/>
<connect gate="-O" pin="IOO13" pad="N35"/>
<connect gate="-O" pin="IOO2" pad="M3"/>
<connect gate="-O" pin="IOO3" pad="M32"/>
<connect gate="-O" pin="IOO4" pad="N1"/>
<connect gate="-O" pin="IOO5" pad="M5"/>
<connect gate="-O" pin="IOO6" pad="M35"/>
<connect gate="-O" pin="IOO7" pad="L35"/>
<connect gate="-O" pin="IOO8" pad="M1"/>
<connect gate="-O" pin="IOO9" pad="M4"/>
<connect gate="-P" pin="IOP1" pad="K35"/>
<connect gate="-P" pin="IOP10" pad="L1"/>
<connect gate="-P" pin="IOP11" pad="L3"/>
<connect gate="-P" pin="IOP12" pad="L4"/>
<connect gate="-P" pin="IOP13" pad="L32"/>
<connect gate="-P" pin="IOP14" pad="L33"/>
<connect gate="-P" pin="IOP2" pad="K1"/>
<connect gate="-P" pin="IOP3" pad="L31"/>
<connect gate="-P" pin="IOP4" pad="L5"/>
<connect gate="-P" pin="IOP5" pad="L34"/>
<connect gate="-P" pin="IOP6" pad="L2"/>
<connect gate="-P" pin="IOP7" pad="K33"/>
<connect gate="-P" pin="IOP8" pad="K2"/>
<connect gate="-P" pin="IOP9" pad="K34"/>
<connect gate="-Q" pin="IOQ1" pad="H35"/>
<connect gate="-Q" pin="IOQ10" pad="K4"/>
<connect gate="-Q" pin="IOQ11" pad="K5"/>
<connect gate="-Q" pin="IOQ12" pad="J1"/>
<connect gate="-Q" pin="IOQ13" pad="J34"/>
<connect gate="-Q" pin="IOQ14" pad="J35"/>
<connect gate="-Q" pin="IOQ2" pad="J2"/>
<connect gate="-Q" pin="IOQ3" pad="J4"/>
<connect gate="-Q" pin="IOQ4" pad="J33"/>
<connect gate="-Q" pin="IOQ5" pad="K31"/>
<connect gate="-Q" pin="IOQ6" pad="K3"/>
<connect gate="-Q" pin="IOQ7" pad="H34"/>
<connect gate="-Q" pin="IOQ8" pad="J3"/>
<connect gate="-Q" pin="IOQ9" pad="J32"/>
<connect gate="-R" pin="IOR1" pad="H4"/>
<connect gate="-R" pin="IOR10" pad="G2"/>
<connect gate="-R" pin="IOR11" pad="H32"/>
<connect gate="-R" pin="IOR12" pad="J31"/>
<connect gate="-R" pin="IOR2" pad="H33"/>
<connect gate="-R" pin="IOR3" pad="H3"/>
<connect gate="-R" pin="IOR4" pad="G34"/>
<connect gate="-R" pin="IOR5" pad="G1"/>
<connect gate="-R" pin="IOR6" pad="G33"/>
<connect gate="-R" pin="IOR7" pad="G35"/>
<connect gate="-R" pin="IOR8" pad="H2"/>
<connect gate="-R" pin="IOR9" pad="J5"/>
<connect gate="-S" pin="IOS1" pad="F3"/>
<connect gate="-S" pin="IOS10" pad="E34"/>
<connect gate="-S" pin="IOS11" pad="F33"/>
<connect gate="-S" pin="IOS12" pad="H31"/>
<connect gate="-S" pin="IOS13" pad="G3"/>
<connect gate="-S" pin="IOS2" pad="E35"/>
<connect gate="-S" pin="IOS3" pad="G32"/>
<connect gate="-S" pin="IOS4" pad="H5"/>
<connect gate="-S" pin="IOS5" pad="F34"/>
<connect gate="-S" pin="IOS6" pad="F1"/>
<connect gate="-S" pin="IOS7" pad="F2"/>
<connect gate="-S" pin="IOS8" pad="G4"/>
<connect gate="-S" pin="IOS9" pad="E1"/>
<connect gate="-T" pin="IOT1" pad="E4"/>
<connect gate="-T" pin="IOT10" pad="D3"/>
<connect gate="-T" pin="IOT11" pad="D35"/>
<connect gate="-T" pin="IOT12" pad="F4"/>
<connect gate="-T" pin="IOT13" pad="D33"/>
<connect gate="-T" pin="IOT14" pad="F32"/>
<connect gate="-T" pin="IOT2" pad="E32"/>
<connect gate="-T" pin="IOT3" pad="D34"/>
<connect gate="-T" pin="IOT4" pad="G5"/>
<connect gate="-T" pin="IOT5" pad="D2"/>
<connect gate="-T" pin="IOT6" pad="G31"/>
<connect gate="-T" pin="IOT7" pad="E33"/>
<connect gate="-T" pin="IOT8" pad="E3"/>
<connect gate="-T" pin="IOT9" pad="D1"/>
<connect gate="G1" pin="GND" pad="AL6"/>
<connect gate="G10" pin="GND" pad="AP2"/>
<connect gate="G11" pin="GND" pad="AP3"/>
<connect gate="G12" pin="GND" pad="AP4"/>
<connect gate="G13" pin="GND" pad="AP5"/>
<connect gate="G14" pin="GND" pad="AP6"/>
<connect gate="G15" pin="GND" pad="AP30"/>
<connect gate="G16" pin="GND" pad="AP31"/>
<connect gate="G17" pin="GND" pad="AP32"/>
<connect gate="G18" pin="GND" pad="AP33"/>
<connect gate="G19" pin="GND" pad="AR1"/>
<connect gate="G2" pin="GND" pad="AL30"/>
<connect gate="G20" pin="GND" pad="AR2"/>
<connect gate="G21" pin="GND" pad="AR3"/>
<connect gate="G22" pin="GND" pad="AR4"/>
<connect gate="G23" pin="GND" pad="AR5"/>
<connect gate="G24" pin="GND" pad="AR30"/>
<connect gate="G25" pin="GND" pad="AR31"/>
<connect gate="G26" pin="GND" pad="AR32"/>
<connect gate="G27" pin="GND" pad="AR33"/>
<connect gate="G28" pin="GND" pad="AR34"/>
<connect gate="G29" pin="GND" pad="AR35"/>
<connect gate="G3" pin="GND" pad="AM6"/>
<connect gate="G30" pin="GND" pad="A1"/>
<connect gate="G31" pin="GND" pad="A2"/>
<connect gate="G32" pin="GND" pad="A3"/>
<connect gate="G33" pin="GND" pad="A4"/>
<connect gate="G34" pin="GND" pad="A5"/>
<connect gate="G35" pin="GND" pad="A18"/>
<connect gate="G36" pin="GND" pad="A31"/>
<connect gate="G37" pin="GND" pad="A32"/>
<connect gate="G38" pin="GND" pad="A33"/>
<connect gate="G39" pin="GND" pad="A34"/>
<connect gate="G4" pin="GND" pad="AM30"/>
<connect gate="G40" pin="GND" pad="A35"/>
<connect gate="G41" pin="GND" pad="B2"/>
<connect gate="G42" pin="GND" pad="B3"/>
<connect gate="G43" pin="GND" pad="B4"/>
<connect gate="G44" pin="GND" pad="B5"/>
<connect gate="G45" pin="GND" pad="B6"/>
<connect gate="G46" pin="GND" pad="B31"/>
<connect gate="G47" pin="GND" pad="B32"/>
<connect gate="G48" pin="GND" pad="B33"/>
<connect gate="G49" pin="GND" pad="B34"/>
<connect gate="G5" pin="GND" pad="AN5"/>
<connect gate="G50" pin="GND" pad="B35"/>
<connect gate="G51" pin="GND" pad="C5"/>
<connect gate="G52" pin="GND" pad="C6"/>
<connect gate="G53" pin="GND" pad="C30"/>
<connect gate="G54" pin="GND" pad="C31"/>
<connect gate="G55" pin="GND" pad="D6"/>
<connect gate="G56" pin="GND" pad="D30"/>
<connect gate="G57" pin="GND" pad="E6"/>
<connect gate="G58" pin="GND" pad="E30"/>
<connect gate="G6" pin="GND" pad="AN6"/>
<connect gate="G7" pin="GND" pad="AN30"/>
<connect gate="G8" pin="GND" pad="AN31"/>
<connect gate="G9" pin="GND" pad="AN35"/>
<connect gate="V1" pin="VCC" pad="AA33"/>
<connect gate="V10" pin="VCC" pad="AP24"/>
<connect gate="V11" pin="VCC" pad="AR11"/>
<connect gate="V12" pin="VCC" pad="AR18"/>
<connect gate="V13" pin="VCC" pad="A11"/>
<connect gate="V14" pin="VCC" pad="A19"/>
<connect gate="V15" pin="VCC" pad="B1"/>
<connect gate="V16" pin="VCC" pad="B18"/>
<connect gate="V17" pin="VCC" pad="D24"/>
<connect gate="V18" pin="VCC" pad="E2"/>
<connect gate="V19" pin="VCC" pad="F31"/>
<connect gate="V2" pin="VCC" pad="AB5"/>
<connect gate="V20" pin="VCC" pad="F35"/>
<connect gate="V21" pin="VCC" pad="H1"/>
<connect gate="V22" pin="VCC" pad="K32"/>
<connect gate="V23" pin="VCC" pad="M2"/>
<connect gate="V24" pin="VCC" pad="N34"/>
<connect gate="V25" pin="VCC" pad="P5"/>
<connect gate="V26" pin="VCC" pad="T35"/>
<connect gate="V27" pin="VCC" pad="U3"/>
<connect gate="V28" pin="VCC" pad="V32"/>
<connect gate="V29" pin="VCC" pad="Y2"/>
<connect gate="V3" pin="VCC" pad="AD35"/>
<connect gate="V4" pin="VCC" pad="AE4"/>
<connect gate="V5" pin="VCC" pad="AF32"/>
<connect gate="V6" pin="VCC" pad="AG5"/>
<connect gate="V7" pin="VCC" pad="AK31"/>
<connect gate="V8" pin="VCC" pad="AK35"/>
<connect gate="V9" pin="VCC" pad="AL3"/>
<connect gate="VO1" pin="VCCIO" pad="AL5"/>
<connect gate="VO10" pin="VCCIO" pad="AN15"/>
<connect gate="VO11" pin="VCCIO" pad="AN32"/>
<connect gate="VO12" pin="VCCIO" pad="AN33"/>
<connect gate="VO13" pin="VCCIO" pad="AP34"/>
<connect gate="VO14" pin="VCCIO" pad="AR23"/>
<connect gate="VO15" pin="VCCIO" pad="A20"/>
<connect gate="VO16" pin="VCCIO" pad="A27"/>
<connect gate="VO17" pin="VCCIO" pad="C2"/>
<connect gate="VO18" pin="VCCIO" pad="C3"/>
<connect gate="VO19" pin="VCCIO" pad="C4"/>
<connect gate="VO2" pin="VCCIO" pad="AL12"/>
<connect gate="VO20" pin="VCCIO" pad="C8"/>
<connect gate="VO21" pin="VCCIO" pad="C15"/>
<connect gate="VO22" pin="VCCIO" pad="C23"/>
<connect gate="VO23" pin="VCCIO" pad="C32"/>
<connect gate="VO24" pin="VCCIO" pad="C33"/>
<connect gate="VO25" pin="VCCIO" pad="D5"/>
<connect gate="VO26" pin="VCCIO" pad="D31"/>
<connect gate="VO27" pin="VCCIO" pad="E5"/>
<connect gate="VO28" pin="VCCIO" pad="E12"/>
<connect gate="VO29" pin="VCCIO" pad="E31"/>
<connect gate="VO3" pin="VCCIO" pad="AM5"/>
<connect gate="VO4" pin="VCCIO" pad="AM19"/>
<connect gate="VO5" pin="VCCIO" pad="AM26"/>
<connect gate="VO6" pin="VCCIO" pad="AM31"/>
<connect gate="VO7" pin="VCCIO" pad="AN3"/>
<connect gate="VO8" pin="VCCIO" pad="AN4"/>
<connect gate="VO9" pin="VCCIO" pad="AN8"/>
<connect gate="_" pin="/CE" pad="AN2"/>
<connect gate="_" pin="/CEO" pad="AP35"/>
<connect gate="_" pin="/CONFIG" pad="D4"/>
<connect gate="_" pin="/STATUS" pad="D32"/>
<connect gate="_" pin="CONF_DONE" pad="AM32"/>
<connect gate="_" pin="DATA0" pad="AM4"/>
<connect gate="_" pin="DCLK" pad="AP1"/>
<connect gate="_" pin="GCLK0" pad="E18"/>
<connect gate="_" pin="GCLK1" pad="AL18"/>
<connect gate="_" pin="IN0" pad="AN18"/>
<connect gate="_" pin="IN1" pad="AM18"/>
<connect gate="_" pin="IN2" pad="C18"/>
<connect gate="_" pin="IN3" pad="D18"/>
<connect gate="_" pin="MSEL0" pad="F5"/>
<connect gate="_" pin="MSEL1" pad="C1"/>
<connect gate="_" pin="TCK" pad="AL31"/>
<connect gate="_" pin="TDI" pad="AN1"/>
<connect gate="_" pin="TDO" pad="AN34"/>
<connect gate="_" pin="TMS" pad="C35"/>
<connect gate="_" pin="TRST" pad="C34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K200-BGA600" prefix="IC">
<description>&lt;b&gt;EPF10K200&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="200B600C"/>
<gate name="-AB" symbol="AB11"/>
<gate name="-CD" symbol="CD11"/>
<gate name="-EF" symbol="EF10"/>
<gate name="-GH" symbol="GH11"/>
<gate name="-IJ" symbol="IJ12"/>
<gate name="-KL" symbol="KL10"/>
<gate name="-MN" symbol="MN11"/>
<gate name="-OP" symbol="OP11"/>
<gate name="-QR" symbol="QR10"/>
<gate name="-ST" symbol="ST11"/>
<gate name="-UV" symbol="UV11"/>
<gate name="-WX" symbol="WX10"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="-10" symbol="IO404"/>
<gate name="-11" symbol="IO444"/>
<gate name="-12" symbol="IO484"/>
<gate name="-13" symbol="IO524"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="G50" symbol="GND"/>
<gate name="G51" symbol="GND"/>
<gate name="G52" symbol="GND"/>
<gate name="G53" symbol="GND"/>
<gate name="G54" symbol="GND"/>
<gate name="G55" symbol="GND"/>
<gate name="G56" symbol="GND"/>
<gate name="G57" symbol="GND"/>
<gate name="G58" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="V24" symbol="VCCINT"/>
<gate name="V25" symbol="VCCINT"/>
<gate name="V26" symbol="VCCINT"/>
<gate name="V27" symbol="VCCINT"/>
<gate name="V28" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="BGA600">
<connects>
<connect gate="-1" pin="IO11" pad="E7"/>
<connect gate="-1" pin="IO12" pad="AR6"/>
<connect gate="-1" pin="IO13" pad="AL7"/>
<connect gate="-1" pin="IO14" pad="A6"/>
<connect gate="-1" pin="IO21" pad="C7"/>
<connect gate="-1" pin="IO22" pad="AM7"/>
<connect gate="-1" pin="IO23" pad="AN7"/>
<connect gate="-1" pin="IO24" pad="D7"/>
<connect gate="-1" pin="IO31" pad="A7"/>
<connect gate="-1" pin="IO32" pad="AP7"/>
<connect gate="-1" pin="IO33" pad="AR7"/>
<connect gate="-1" pin="IO34" pad="B7"/>
<connect gate="-1" pin="IO41" pad="D8"/>
<connect gate="-1" pin="IO42" pad="AL8"/>
<connect gate="-1" pin="IO43" pad="AM8"/>
<connect gate="-1" pin="IO44" pad="E8"/>
<connect gate="-10" pin="IO371" pad="AN23"/>
<connect gate="-10" pin="IO372" pad="AP23"/>
<connect gate="-10" pin="IO373" pad="E23"/>
<connect gate="-10" pin="IO374" pad="D23"/>
<connect gate="-10" pin="IO381" pad="B24"/>
<connect gate="-10" pin="IO382" pad="AL23"/>
<connect gate="-10" pin="IO383" pad="AM23"/>
<connect gate="-10" pin="IO384" pad="A24"/>
<connect gate="-10" pin="IO391" pad="A25"/>
<connect gate="-10" pin="IO392" pad="AR24"/>
<connect gate="-10" pin="IO393" pad="AN24"/>
<connect gate="-10" pin="IO394" pad="C24"/>
<connect gate="-10" pin="IO401" pad="AR25"/>
<connect gate="-10" pin="IO402" pad="E24"/>
<connect gate="-10" pin="IO403" pad="AM24"/>
<connect gate="-10" pin="IO404" pad="B25"/>
<connect gate="-11" pin="IO411" pad="C25"/>
<connect gate="-11" pin="IO412" pad="AL24"/>
<connect gate="-11" pin="IO413" pad="AP25"/>
<connect gate="-11" pin="IO414" pad="D25"/>
<connect gate="-11" pin="IO421" pad="A26"/>
<connect gate="-11" pin="IO422" pad="AM25"/>
<connect gate="-11" pin="IO423" pad="AN25"/>
<connect gate="-11" pin="IO424" pad="E25"/>
<connect gate="-11" pin="IO431" pad="B26"/>
<connect gate="-11" pin="IO432" pad="AR26"/>
<connect gate="-11" pin="IO433" pad="AL25"/>
<connect gate="-11" pin="IO434" pad="C26"/>
<connect gate="-11" pin="IO441" pad="E26"/>
<connect gate="-11" pin="IO442" pad="AN26"/>
<connect gate="-11" pin="IO443" pad="AP26"/>
<connect gate="-11" pin="IO444" pad="D26"/>
<connect gate="-12" pin="IO451" pad="C27"/>
<connect gate="-12" pin="IO452" pad="AL26"/>
<connect gate="-12" pin="IO453" pad="AR27"/>
<connect gate="-12" pin="IO454" pad="B27"/>
<connect gate="-12" pin="IO461" pad="E27"/>
<connect gate="-12" pin="IO462" pad="AN27"/>
<connect gate="-12" pin="IO463" pad="AP27"/>
<connect gate="-12" pin="IO464" pad="D27"/>
<connect gate="-12" pin="IO471" pad="B28"/>
<connect gate="-12" pin="IO472" pad="AL27"/>
<connect gate="-12" pin="IO473" pad="AM27"/>
<connect gate="-12" pin="IO474" pad="A28"/>
<connect gate="-12" pin="IO481" pad="D28"/>
<connect gate="-12" pin="IO482" pad="AP28"/>
<connect gate="-12" pin="IO483" pad="AR28"/>
<connect gate="-12" pin="IO484" pad="C28"/>
<connect gate="-13" pin="IO491" pad="A29"/>
<connect gate="-13" pin="IO492" pad="AM28"/>
<connect gate="-13" pin="IO493" pad="AN28"/>
<connect gate="-13" pin="IO494" pad="E28"/>
<connect gate="-13" pin="IO501" pad="AL28"/>
<connect gate="-13" pin="IO502" pad="AR29"/>
<connect gate="-13" pin="IO503" pad="B29"/>
<connect gate="-13" pin="IO504" pad="C29"/>
<connect gate="-13" pin="IO511" pad="E29"/>
<connect gate="-13" pin="IO512" pad="AN29"/>
<connect gate="-13" pin="IO513" pad="AP29"/>
<connect gate="-13" pin="IO514" pad="D29"/>
<connect gate="-13" pin="IO521" pad="B30"/>
<connect gate="-13" pin="IO522" pad="AL29"/>
<connect gate="-13" pin="IO523" pad="AM29"/>
<connect gate="-13" pin="IO524" pad="A30"/>
<connect gate="-2" pin="IO51" pad="A8"/>
<connect gate="-2" pin="IO52" pad="B8"/>
<connect gate="-2" pin="IO53" pad="AR8"/>
<connect gate="-2" pin="IO54" pad="AP8"/>
<connect gate="-2" pin="IO61" pad="D9"/>
<connect gate="-2" pin="IO62" pad="AM9"/>
<connect gate="-2" pin="IO63" pad="AL9"/>
<connect gate="-2" pin="IO64" pad="E9"/>
<connect gate="-2" pin="IO71" pad="B9"/>
<connect gate="-2" pin="IO72" pad="AP9"/>
<connect gate="-2" pin="IO73" pad="AN9"/>
<connect gate="-2" pin="IO74" pad="C9"/>
<connect gate="-2" pin="IO81" pad="E10"/>
<connect gate="-2" pin="IO82" pad="A9"/>
<connect gate="-2" pin="IO83" pad="AL10"/>
<connect gate="-2" pin="IO84" pad="AR9"/>
<connect gate="-3" pin="IO101" pad="A10"/>
<connect gate="-3" pin="IO102" pad="AR10"/>
<connect gate="-3" pin="IO103" pad="AP10"/>
<connect gate="-3" pin="IO104" pad="B10"/>
<connect gate="-3" pin="IO111" pad="D11"/>
<connect gate="-3" pin="IO112" pad="AM11"/>
<connect gate="-3" pin="IO113" pad="AL11"/>
<connect gate="-3" pin="IO114" pad="E11"/>
<connect gate="-3" pin="IO121" pad="B11"/>
<connect gate="-3" pin="IO122" pad="AN11"/>
<connect gate="-3" pin="IO123" pad="AP11"/>
<connect gate="-3" pin="IO124" pad="C11"/>
<connect gate="-3" pin="IO91" pad="C10"/>
<connect gate="-3" pin="IO92" pad="AN10"/>
<connect gate="-3" pin="IO93" pad="AM10"/>
<connect gate="-3" pin="IO94" pad="D10"/>
<connect gate="-4" pin="IO131" pad="D12"/>
<connect gate="-4" pin="IO132" pad="AN12"/>
<connect gate="-4" pin="IO133" pad="AM12"/>
<connect gate="-4" pin="IO134" pad="C12"/>
<connect gate="-4" pin="IO141" pad="B12"/>
<connect gate="-4" pin="IO142" pad="AR12"/>
<connect gate="-4" pin="IO143" pad="AP12"/>
<connect gate="-4" pin="IO144" pad="A12"/>
<connect gate="-4" pin="IO151" pad="E13"/>
<connect gate="-4" pin="IO152" pad="AM13"/>
<connect gate="-4" pin="IO153" pad="AL13"/>
<connect gate="-4" pin="IO154" pad="D13"/>
<connect gate="-4" pin="IO161" pad="C13"/>
<connect gate="-4" pin="IO162" pad="AP13"/>
<connect gate="-4" pin="IO163" pad="AN13"/>
<connect gate="-4" pin="IO164" pad="B13"/>
<connect gate="-5" pin="IO171" pad="E14"/>
<connect gate="-5" pin="IO172" pad="AL14"/>
<connect gate="-5" pin="IO173" pad="AR13"/>
<connect gate="-5" pin="IO174" pad="A13"/>
<connect gate="-5" pin="IO181" pad="C14"/>
<connect gate="-5" pin="IO182" pad="AN14"/>
<connect gate="-5" pin="IO183" pad="AM14"/>
<connect gate="-5" pin="IO184" pad="D14"/>
<connect gate="-5" pin="IO191" pad="A14"/>
<connect gate="-5" pin="IO192" pad="AR14"/>
<connect gate="-5" pin="IO193" pad="AP14"/>
<connect gate="-5" pin="IO194" pad="B14"/>
<connect gate="-5" pin="IO201" pad="D15"/>
<connect gate="-5" pin="IO202" pad="AM15"/>
<connect gate="-5" pin="IO203" pad="AL15"/>
<connect gate="-5" pin="IO204" pad="E15"/>
<connect gate="-6" pin="IO211" pad="A15"/>
<connect gate="-6" pin="IO212" pad="AP15"/>
<connect gate="-6" pin="IO213" pad="AR15"/>
<connect gate="-6" pin="IO214" pad="B15"/>
<connect gate="-6" pin="IO221" pad="D16"/>
<connect gate="-6" pin="IO222" pad="AL16"/>
<connect gate="-6" pin="IO223" pad="AM16"/>
<connect gate="-6" pin="IO224" pad="E16"/>
<connect gate="-6" pin="IO231" pad="B16"/>
<connect gate="-6" pin="IO232" pad="AN16"/>
<connect gate="-6" pin="IO233" pad="AP16"/>
<connect gate="-6" pin="IO234" pad="C16"/>
<connect gate="-6" pin="IO241" pad="E17"/>
<connect gate="-6" pin="IO242" pad="AR16"/>
<connect gate="-6" pin="IO243" pad="AL17"/>
<connect gate="-6" pin="IO244" pad="A16"/>
<connect gate="-7" pin="IO251" pad="AM17"/>
<connect gate="-7" pin="IO252" pad="AN17"/>
<connect gate="-7" pin="IO253" pad="C17"/>
<connect gate="-7" pin="IO254" pad="D17"/>
<connect gate="-7" pin="IO261" pad="AP17"/>
<connect gate="-7" pin="IO262" pad="AR17"/>
<connect gate="-7" pin="IO263" pad="A17"/>
<connect gate="-7" pin="IO264" pad="B17"/>
<connect gate="-7" pin="IO271" pad="C19"/>
<connect gate="-7" pin="IO272" pad="AR19"/>
<connect gate="-7" pin="IO273" pad="AP18"/>
<connect gate="-7" pin="IO274" pad="B19"/>
<connect gate="-7" pin="IO281" pad="E19"/>
<connect gate="-7" pin="IO282" pad="D19"/>
<connect gate="-7" pin="IO283" pad="AP19"/>
<connect gate="-7" pin="IO284" pad="AN19"/>
<connect gate="-8" pin="IO291" pad="C20"/>
<connect gate="-8" pin="IO292" pad="AL19"/>
<connect gate="-8" pin="IO293" pad="AR20"/>
<connect gate="-8" pin="IO294" pad="B20"/>
<connect gate="-8" pin="IO301" pad="E20"/>
<connect gate="-8" pin="IO302" pad="AN20"/>
<connect gate="-8" pin="IO303" pad="AP20"/>
<connect gate="-8" pin="IO304" pad="D20"/>
<connect gate="-8" pin="IO311" pad="B21"/>
<connect gate="-8" pin="IO312" pad="AL20"/>
<connect gate="-8" pin="IO313" pad="AM20"/>
<connect gate="-8" pin="IO314" pad="A21"/>
<connect gate="-8" pin="IO321" pad="D21"/>
<connect gate="-8" pin="IO322" pad="AP21"/>
<connect gate="-8" pin="IO323" pad="AR21"/>
<connect gate="-8" pin="IO324" pad="C21"/>
<connect gate="-9" pin="IO331" pad="A22"/>
<connect gate="-9" pin="IO332" pad="AM21"/>
<connect gate="-9" pin="IO333" pad="AN21"/>
<connect gate="-9" pin="IO334" pad="E21"/>
<connect gate="-9" pin="IO341" pad="C22"/>
<connect gate="-9" pin="IO342" pad="AR22"/>
<connect gate="-9" pin="IO343" pad="AL21"/>
<connect gate="-9" pin="IO344" pad="B22"/>
<connect gate="-9" pin="IO351" pad="E22"/>
<connect gate="-9" pin="IO352" pad="AN22"/>
<connect gate="-9" pin="IO353" pad="D22"/>
<connect gate="-9" pin="IO354" pad="AP22"/>
<connect gate="-9" pin="IO361" pad="A23"/>
<connect gate="-9" pin="IO362" pad="B23"/>
<connect gate="-9" pin="IO363" pad="AL22"/>
<connect gate="-9" pin="IO364" pad="AM22"/>
<connect gate="-AB" pin="IOA1" pad="AL32"/>
<connect gate="-AB" pin="IOA10" pad="AL4"/>
<connect gate="-AB" pin="IOA11" pad="AM2"/>
<connect gate="-AB" pin="IOA2" pad="AM33"/>
<connect gate="-AB" pin="IOA3" pad="AM34"/>
<connect gate="-AB" pin="IOA4" pad="AK5"/>
<connect gate="-AB" pin="IOA5" pad="AM1"/>
<connect gate="-AB" pin="IOA6" pad="AM3"/>
<connect gate="-AB" pin="IOA7" pad="AJ31"/>
<connect gate="-AB" pin="IOA8" pad="AJ5"/>
<connect gate="-AB" pin="IOA9" pad="AM35"/>
<connect gate="-AB" pin="IOB1" pad="AK32"/>
<connect gate="-AB" pin="IOB10" pad="AK3"/>
<connect gate="-AB" pin="IOB11" pad="AL34"/>
<connect gate="-AB" pin="IOB2" pad="AL33"/>
<connect gate="-AB" pin="IOB3" pad="AL1"/>
<connect gate="-AB" pin="IOB4" pad="AK4"/>
<connect gate="-AB" pin="IOB5" pad="AJ4"/>
<connect gate="-AB" pin="IOB6" pad="AL35"/>
<connect gate="-AB" pin="IOB7" pad="AJ32"/>
<connect gate="-AB" pin="IOB8" pad="AL2"/>
<connect gate="-AB" pin="IOB9" pad="AK33"/>
<connect gate="-CD" pin="IOC1" pad="AK34"/>
<connect gate="-CD" pin="IOC10" pad="AJ35"/>
<connect gate="-CD" pin="IOC2" pad="AJ33"/>
<connect gate="-CD" pin="IOC3" pad="AJ2"/>
<connect gate="-CD" pin="IOC4" pad="AK2"/>
<connect gate="-CD" pin="IOC5" pad="AJ3"/>
<connect gate="-CD" pin="IOC6" pad="AJ34"/>
<connect gate="-CD" pin="IOC7" pad="AK1"/>
<connect gate="-CD" pin="IOC8" pad="AH31"/>
<connect gate="-CD" pin="IOC9" pad="AH5"/>
<connect gate="-CD" pin="IOD1" pad="AH34"/>
<connect gate="-CD" pin="IOD10" pad="AG31"/>
<connect gate="-CD" pin="IOD11" pad="AH4"/>
<connect gate="-CD" pin="IOD2" pad="AH35"/>
<connect gate="-CD" pin="IOD3" pad="AH1"/>
<connect gate="-CD" pin="IOD4" pad="AH2"/>
<connect gate="-CD" pin="IOD5" pad="AH3"/>
<connect gate="-CD" pin="IOD6" pad="AH33"/>
<connect gate="-CD" pin="IOD7" pad="AJ1"/>
<connect gate="-CD" pin="IOD8" pad="AH32"/>
<connect gate="-CD" pin="IOD9" pad="AG4"/>
<connect gate="-EF" pin="IOE1" pad="AF31"/>
<connect gate="-EF" pin="IOE10" pad="AG35"/>
<connect gate="-EF" pin="IOE11" pad="AG34"/>
<connect gate="-EF" pin="IOE2" pad="AG1"/>
<connect gate="-EF" pin="IOE3" pad="AF4"/>
<connect gate="-EF" pin="IOE4" pad="AF5"/>
<connect gate="-EF" pin="IOE5" pad="AG2"/>
<connect gate="-EF" pin="IOE6" pad="AG32"/>
<connect gate="-EF" pin="IOE7" pad="AF33"/>
<connect gate="-EF" pin="IOE8" pad="AG3"/>
<connect gate="-EF" pin="IOE9" pad="AG33"/>
<connect gate="-EF" pin="IOF1" pad="AF35"/>
<connect gate="-EF" pin="IOF10" pad="AF3"/>
<connect gate="-EF" pin="IOF2" pad="AE31"/>
<connect gate="-EF" pin="IOF3" pad="AE5"/>
<connect gate="-EF" pin="IOF4" pad="AE32"/>
<connect gate="-EF" pin="IOF5" pad="AF2"/>
<connect gate="-EF" pin="IOF6" pad="AE33"/>
<connect gate="-EF" pin="IOF7" pad="AE3"/>
<connect gate="-EF" pin="IOF8" pad="AF1"/>
<connect gate="-EF" pin="IOF9" pad="AF34"/>
<connect gate="-GH" pin="IOG1" pad="AD31"/>
<connect gate="-GH" pin="IOG10" pad="AE35"/>
<connect gate="-GH" pin="IOG11" pad="AE1"/>
<connect gate="-GH" pin="IOG2" pad="AD5"/>
<connect gate="-GH" pin="IOG3" pad="AD3"/>
<connect gate="-GH" pin="IOG4" pad="AD33"/>
<connect gate="-GH" pin="IOG5" pad="AE2"/>
<connect gate="-GH" pin="IOG6" pad="AE34"/>
<connect gate="-GH" pin="IOG7" pad="AD2"/>
<connect gate="-GH" pin="IOG8" pad="AD32"/>
<connect gate="-GH" pin="IOG9" pad="AD4"/>
<connect gate="-GH" pin="IOH1" pad="AC4"/>
<connect gate="-GH" pin="IOH10" pad="AC32"/>
<connect gate="-GH" pin="IOH11" pad="AC34"/>
<connect gate="-GH" pin="IOH2" pad="AC5"/>
<connect gate="-GH" pin="IOH3" pad="AD1"/>
<connect gate="-GH" pin="IOH4" pad="AC2"/>
<connect gate="-GH" pin="IOH5" pad="AD34"/>
<connect gate="-GH" pin="IOH6" pad="AC33"/>
<connect gate="-GH" pin="IOH7" pad="AC35"/>
<connect gate="-GH" pin="IOH8" pad="AC31"/>
<connect gate="-GH" pin="IOH9" pad="AC3"/>
<connect gate="-IJ" pin="IOI10" pad="AB31"/>
<connect gate="-IJ" pin="IOI11" pad="AC1"/>
<connect gate="-IJ" pin="IOI2" pad="AB32"/>
<connect gate="-IJ" pin="IOI3" pad="AB2"/>
<connect gate="-IJ" pin="IOI4" pad="AB34"/>
<connect gate="-IJ" pin="IOI5" pad="AB4"/>
<connect gate="-IJ" pin="IOI6" pad="AB1"/>
<connect gate="-IJ" pin="IOI7" pad="AB33"/>
<connect gate="-IJ" pin="IOI8" pad="AB35"/>
<connect gate="-IJ" pin="IOI9" pad="AB3"/>
<connect gate="-IJ" pin="IOJ1" pad="AA31"/>
<connect gate="-IJ" pin="IOJ10" pad="AA35"/>
<connect gate="-IJ" pin="IOJ11" pad="AA32"/>
<connect gate="-IJ" pin="IOJ12" pad="AA4"/>
<connect gate="-IJ" pin="IOJ3" pad="AA1"/>
<connect gate="-IJ" pin="IOJ4" pad="AA2"/>
<connect gate="-IJ" pin="IOJ5" pad="AA3"/>
<connect gate="-IJ" pin="IOJ6" pad="AA34"/>
<connect gate="-IJ" pin="IOJ7" pad="AA5"/>
<connect gate="-IJ" pin="IOJ8" pad="Y31"/>
<connect gate="-IJ" pin="IOJ9" pad="Y5"/>
<connect gate="-KL" pin="IOK1" pad="Y34"/>
<connect gate="-KL" pin="IOK10" pad="Y3"/>
<connect gate="-KL" pin="IOK11" pad="Y32"/>
<connect gate="-KL" pin="IOK2" pad="Y35"/>
<connect gate="-KL" pin="IOK3" pad="W4"/>
<connect gate="-KL" pin="IOK4" pad="W5"/>
<connect gate="-KL" pin="IOK5" pad="Y1"/>
<connect gate="-KL" pin="IOK6" pad="Y4"/>
<connect gate="-KL" pin="IOK7" pad="Y33"/>
<connect gate="-KL" pin="IOK8" pad="W32"/>
<connect gate="-KL" pin="IOK9" pad="W31"/>
<connect gate="-KL" pin="IOL1" pad="W35"/>
<connect gate="-KL" pin="IOL10" pad="W3"/>
<connect gate="-KL" pin="IOL2" pad="V31"/>
<connect gate="-KL" pin="IOL3" pad="V4"/>
<connect gate="-KL" pin="IOL4" pad="V33"/>
<connect gate="-KL" pin="IOL5" pad="W1"/>
<connect gate="-KL" pin="IOL6" pad="V5"/>
<connect gate="-KL" pin="IOL7" pad="W2"/>
<connect gate="-KL" pin="IOL8" pad="W34"/>
<connect gate="-KL" pin="IOL9" pad="W33"/>
<connect gate="-MN" pin="IOM1" pad="V35"/>
<connect gate="-MN" pin="IOM10" pad="V3"/>
<connect gate="-MN" pin="IOM11" pad="V34"/>
<connect gate="-MN" pin="IOM2" pad="U31"/>
<connect gate="-MN" pin="IOM3" pad="U5"/>
<connect gate="-MN" pin="IOM4" pad="U2"/>
<connect gate="-MN" pin="IOM5" pad="V1"/>
<connect gate="-MN" pin="IOM6" pad="U4"/>
<connect gate="-MN" pin="IOM7" pad="U33"/>
<connect gate="-MN" pin="IOM8" pad="U32"/>
<connect gate="-MN" pin="IOM9" pad="V2"/>
<connect gate="-MN" pin="ION1" pad="U35"/>
<connect gate="-MN" pin="ION10" pad="U34"/>
<connect gate="-MN" pin="ION11" pad="T33"/>
<connect gate="-MN" pin="ION2" pad="T32"/>
<connect gate="-MN" pin="ION3" pad="T4"/>
<connect gate="-MN" pin="ION4" pad="T5"/>
<connect gate="-MN" pin="ION5" pad="T3"/>
<connect gate="-MN" pin="ION6" pad="T31"/>
<connect gate="-MN" pin="ION7" pad="U1"/>
<connect gate="-MN" pin="ION8" pad="T2"/>
<connect gate="-MN" pin="ION9" pad="T34"/>
<connect gate="-OP" pin="IOO1" pad="R32"/>
<connect gate="-OP" pin="IOO10" pad="R34"/>
<connect gate="-OP" pin="IOO2" pad="R3"/>
<connect gate="-OP" pin="IOO3" pad="R4"/>
<connect gate="-OP" pin="IOO4" pad="R5"/>
<connect gate="-OP" pin="IOO5" pad="R35"/>
<connect gate="-OP" pin="IOO6" pad="R2"/>
<connect gate="-OP" pin="IOO7" pad="R33"/>
<connect gate="-OP" pin="IOO8" pad="R31"/>
<connect gate="-OP" pin="IOO9" pad="T1"/>
<connect gate="-OP" pin="IOP1" pad="P32"/>
<connect gate="-OP" pin="IOP10" pad="P31"/>
<connect gate="-OP" pin="IOP11" pad="P33"/>
<connect gate="-OP" pin="IOP2" pad="P2"/>
<connect gate="-OP" pin="IOP3" pad="P3"/>
<connect gate="-OP" pin="IOP4" pad="N5"/>
<connect gate="-OP" pin="IOP5" pad="P34"/>
<connect gate="-OP" pin="IOP6" pad="P4"/>
<connect gate="-OP" pin="IOP7" pad="P1"/>
<connect gate="-OP" pin="IOP8" pad="P35"/>
<connect gate="-OP" pin="IOP9" pad="R1"/>
<connect gate="-QR" pin="IOQ1" pad="N35"/>
<connect gate="-QR" pin="IOQ10" pad="N31"/>
<connect gate="-QR" pin="IOQ11" pad="N32"/>
<connect gate="-QR" pin="IOQ2" pad="N1"/>
<connect gate="-QR" pin="IOQ3" pad="N2"/>
<connect gate="-QR" pin="IOQ4" pad="M35"/>
<connect gate="-QR" pin="IOQ5" pad="N33"/>
<connect gate="-QR" pin="IOQ6" pad="M1"/>
<connect gate="-QR" pin="IOQ7" pad="M31"/>
<connect gate="-QR" pin="IOQ8" pad="N4"/>
<connect gate="-QR" pin="IOQ9" pad="N3"/>
<connect gate="-QR" pin="IOR1" pad="M34"/>
<connect gate="-QR" pin="IOR10" pad="M33"/>
<connect gate="-QR" pin="IOR2" pad="L35"/>
<connect gate="-QR" pin="IOR3" pad="L34"/>
<connect gate="-QR" pin="IOR4" pad="L2"/>
<connect gate="-QR" pin="IOR5" pad="M3"/>
<connect gate="-QR" pin="IOR6" pad="M32"/>
<connect gate="-QR" pin="IOR7" pad="M5"/>
<connect gate="-QR" pin="IOR8" pad="L1"/>
<connect gate="-QR" pin="IOR9" pad="M4"/>
<connect gate="-ST" pin="IOS1" pad="K35"/>
<connect gate="-ST" pin="IOS10" pad="L32"/>
<connect gate="-ST" pin="IOS11" pad="L33"/>
<connect gate="-ST" pin="IOS2" pad="K34"/>
<connect gate="-ST" pin="IOS3" pad="L4"/>
<connect gate="-ST" pin="IOS4" pad="K3"/>
<connect gate="-ST" pin="IOS5" pad="K1"/>
<connect gate="-ST" pin="IOS6" pad="L31"/>
<connect gate="-ST" pin="IOS7" pad="L5"/>
<connect gate="-ST" pin="IOS8" pad="K2"/>
<connect gate="-ST" pin="IOS9" pad="L3"/>
<connect gate="-ST" pin="IOT1" pad="J34"/>
<connect gate="-ST" pin="IOT10" pad="K33"/>
<connect gate="-ST" pin="IOT11" pad="J35"/>
<connect gate="-ST" pin="IOT2" pad="K5"/>
<connect gate="-ST" pin="IOT3" pad="J1"/>
<connect gate="-ST" pin="IOT4" pad="J2"/>
<connect gate="-ST" pin="IOT5" pad="J33"/>
<connect gate="-ST" pin="IOT6" pad="K31"/>
<connect gate="-ST" pin="IOT7" pad="J3"/>
<connect gate="-ST" pin="IOT8" pad="J32"/>
<connect gate="-ST" pin="IOT9" pad="K4"/>
<connect gate="-UV" pin="IOU1" pad="H33"/>
<connect gate="-UV" pin="IOU10" pad="H34"/>
<connect gate="-UV" pin="IOU2" pad="J31"/>
<connect gate="-UV" pin="IOU3" pad="H3"/>
<connect gate="-UV" pin="IOU4" pad="H2"/>
<connect gate="-UV" pin="IOU5" pad="H4"/>
<connect gate="-UV" pin="IOU6" pad="H35"/>
<connect gate="-UV" pin="IOU7" pad="J4"/>
<connect gate="-UV" pin="IOU8" pad="J5"/>
<connect gate="-UV" pin="IOU9" pad="H32"/>
<connect gate="-UV" pin="IOV1" pad="G33"/>
<connect gate="-UV" pin="IOV10" pad="G35"/>
<connect gate="-UV" pin="IOV11" pad="G2"/>
<connect gate="-UV" pin="IOV2" pad="F34"/>
<connect gate="-UV" pin="IOV3" pad="F1"/>
<connect gate="-UV" pin="IOV4" pad="G3"/>
<connect gate="-UV" pin="IOV5" pad="H5"/>
<connect gate="-UV" pin="IOV6" pad="G34"/>
<connect gate="-UV" pin="IOV7" pad="F2"/>
<connect gate="-UV" pin="IOV8" pad="H31"/>
<connect gate="-UV" pin="IOV9" pad="G1"/>
<connect gate="-WX" pin="IOW1" pad="G32"/>
<connect gate="-WX" pin="IOW10" pad="E34"/>
<connect gate="-WX" pin="IOW11" pad="F33"/>
<connect gate="-WX" pin="IOW2" pad="E3"/>
<connect gate="-WX" pin="IOW3" pad="E1"/>
<connect gate="-WX" pin="IOW4" pad="E33"/>
<connect gate="-WX" pin="IOW5" pad="F3"/>
<connect gate="-WX" pin="IOW6" pad="E35"/>
<connect gate="-WX" pin="IOW7" pad="F4"/>
<connect gate="-WX" pin="IOW8" pad="F32"/>
<connect gate="-WX" pin="IOW9" pad="G4"/>
<connect gate="-WX" pin="IOX1" pad="G31"/>
<connect gate="-WX" pin="IOX10" pad="D33"/>
<connect gate="-WX" pin="IOX2" pad="D35"/>
<connect gate="-WX" pin="IOX3" pad="D3"/>
<connect gate="-WX" pin="IOX4" pad="D2"/>
<connect gate="-WX" pin="IOX5" pad="E4"/>
<connect gate="-WX" pin="IOX6" pad="E32"/>
<connect gate="-WX" pin="IOX7" pad="D34"/>
<connect gate="-WX" pin="IOX8" pad="G5"/>
<connect gate="-WX" pin="IOX9" pad="D1"/>
<connect gate="G1" pin="GND" pad="AL6"/>
<connect gate="G10" pin="GND" pad="AP5"/>
<connect gate="G11" pin="GND" pad="AP6"/>
<connect gate="G12" pin="GND" pad="AP30"/>
<connect gate="G13" pin="GND" pad="AP31"/>
<connect gate="G14" pin="GND" pad="AP32"/>
<connect gate="G15" pin="GND" pad="AP33"/>
<connect gate="G16" pin="GND" pad="AR1"/>
<connect gate="G17" pin="GND" pad="AR2"/>
<connect gate="G18" pin="GND" pad="AR3"/>
<connect gate="G19" pin="GND" pad="AR4"/>
<connect gate="G2" pin="GND" pad="AL30"/>
<connect gate="G20" pin="GND" pad="AR5"/>
<connect gate="G21" pin="GND" pad="AR30"/>
<connect gate="G22" pin="GND" pad="AR31"/>
<connect gate="G23" pin="GND" pad="AR32"/>
<connect gate="G24" pin="GND" pad="AR33"/>
<connect gate="G25" pin="GND" pad="AR34"/>
<connect gate="G26" pin="GND" pad="AR35"/>
<connect gate="G27" pin="GND" pad="A1"/>
<connect gate="G28" pin="GND" pad="A2"/>
<connect gate="G29" pin="GND" pad="A3"/>
<connect gate="G3" pin="GND" pad="AM6"/>
<connect gate="G30" pin="GND" pad="A4"/>
<connect gate="G31" pin="GND" pad="A5"/>
<connect gate="G32" pin="GND" pad="A18"/>
<connect gate="G33" pin="GND" pad="A31"/>
<connect gate="G34" pin="GND" pad="A32"/>
<connect gate="G35" pin="GND" pad="A33"/>
<connect gate="G36" pin="GND" pad="A34"/>
<connect gate="G37" pin="GND" pad="A35"/>
<connect gate="G38" pin="GND" pad="B2"/>
<connect gate="G39" pin="GND" pad="B3"/>
<connect gate="G4" pin="GND" pad="AM30"/>
<connect gate="G40" pin="GND" pad="B4"/>
<connect gate="G41" pin="GND" pad="B5"/>
<connect gate="G42" pin="GND" pad="B6"/>
<connect gate="G43" pin="GND" pad="B31"/>
<connect gate="G44" pin="GND" pad="B32"/>
<connect gate="G45" pin="GND" pad="B33"/>
<connect gate="G46" pin="GND" pad="B34"/>
<connect gate="G47" pin="GND" pad="B35"/>
<connect gate="G48" pin="GND" pad="C5"/>
<connect gate="G49" pin="GND" pad="C6"/>
<connect gate="G5" pin="GND" pad="AN31"/>
<connect gate="G50" pin="GND" pad="C30"/>
<connect gate="G51" pin="GND" pad="C31"/>
<connect gate="G52" pin="GND" pad="D6"/>
<connect gate="G53" pin="GND" pad="D30"/>
<connect gate="G54" pin="GND" pad="E6"/>
<connect gate="G55" pin="GND" pad="E30"/>
<connect gate="G56" pin="GND" pad="AN5"/>
<connect gate="G57" pin="GND" pad="AN6"/>
<connect gate="G58" pin="GND" pad="AN30"/>
<connect gate="G6" pin="GND" pad="AN35"/>
<connect gate="G7" pin="GND" pad="AP2"/>
<connect gate="G8" pin="GND" pad="AP3"/>
<connect gate="G9" pin="GND" pad="AP4"/>
<connect gate="V1" pin="VCC" pad="AA33"/>
<connect gate="V10" pin="VCC" pad="AP24"/>
<connect gate="V11" pin="VCC" pad="AR11"/>
<connect gate="V12" pin="VCC" pad="AR18"/>
<connect gate="V13" pin="VCC" pad="A11"/>
<connect gate="V14" pin="VCC" pad="A19"/>
<connect gate="V15" pin="VCC" pad="B1"/>
<connect gate="V16" pin="VCC" pad="B18"/>
<connect gate="V17" pin="VCC" pad="D24"/>
<connect gate="V18" pin="VCC" pad="E2"/>
<connect gate="V19" pin="VCC" pad="F31"/>
<connect gate="V2" pin="VCC" pad="AB5"/>
<connect gate="V20" pin="VCC" pad="F35"/>
<connect gate="V21" pin="VCC" pad="H1"/>
<connect gate="V22" pin="VCC" pad="K32"/>
<connect gate="V23" pin="VCC" pad="M2"/>
<connect gate="V24" pin="VCC" pad="N34"/>
<connect gate="V25" pin="VCC" pad="T35"/>
<connect gate="V26" pin="VCC" pad="U3"/>
<connect gate="V27" pin="VCC" pad="V32"/>
<connect gate="V28" pin="VCC" pad="Y2"/>
<connect gate="V3" pin="VCC" pad="AD35"/>
<connect gate="V4" pin="VCC" pad="AE4"/>
<connect gate="V5" pin="VCC" pad="AF32"/>
<connect gate="V6" pin="VCC" pad="AG5"/>
<connect gate="V7" pin="VCC" pad="AK31"/>
<connect gate="V8" pin="VCC" pad="AK35"/>
<connect gate="V9" pin="VCC" pad="AL3"/>
<connect gate="VO1" pin="VCCIO" pad="AL5"/>
<connect gate="VO10" pin="VCCIO" pad="AN15"/>
<connect gate="VO11" pin="VCCIO" pad="AN32"/>
<connect gate="VO12" pin="VCCIO" pad="AN33"/>
<connect gate="VO13" pin="VCCIO" pad="AP34"/>
<connect gate="VO14" pin="VCCIO" pad="AR23"/>
<connect gate="VO15" pin="VCCIO" pad="A20"/>
<connect gate="VO16" pin="VCCIO" pad="A27"/>
<connect gate="VO17" pin="VCCIO" pad="C2"/>
<connect gate="VO18" pin="VCCIO" pad="C3"/>
<connect gate="VO19" pin="VCCIO" pad="C4"/>
<connect gate="VO2" pin="VCCIO" pad="AL12"/>
<connect gate="VO20" pin="VCCIO" pad="C8"/>
<connect gate="VO21" pin="VCCIO" pad="C15"/>
<connect gate="VO22" pin="VCCIO" pad="C23"/>
<connect gate="VO23" pin="VCCIO" pad="C32"/>
<connect gate="VO24" pin="VCCIO" pad="C33"/>
<connect gate="VO25" pin="VCCIO" pad="D5"/>
<connect gate="VO26" pin="VCCIO" pad="D31"/>
<connect gate="VO27" pin="VCCIO" pad="E5"/>
<connect gate="VO28" pin="VCCIO" pad="E12"/>
<connect gate="VO29" pin="VCCIO" pad="E31"/>
<connect gate="VO3" pin="VCCIO" pad="AM5"/>
<connect gate="VO4" pin="VCCIO" pad="AM19"/>
<connect gate="VO5" pin="VCCIO" pad="AM26"/>
<connect gate="VO6" pin="VCCIO" pad="AM31"/>
<connect gate="VO7" pin="VCCIO" pad="AN3"/>
<connect gate="VO8" pin="VCCIO" pad="AN4"/>
<connect gate="VO9" pin="VCCIO" pad="AN8"/>
<connect gate="_" pin="/CE" pad="AN2"/>
<connect gate="_" pin="/CEO" pad="AP35"/>
<connect gate="_" pin="/CONFIG" pad="D4"/>
<connect gate="_" pin="/STATUS" pad="D32"/>
<connect gate="_" pin="CONF_DONE" pad="AM32"/>
<connect gate="_" pin="DATA0" pad="AM4"/>
<connect gate="_" pin="DCLK" pad="AP1"/>
<connect gate="_" pin="GCLK" pad="AL18"/>
<connect gate="_" pin="GCLK1" pad="E18"/>
<connect gate="_" pin="IN0" pad="D18"/>
<connect gate="_" pin="IN1" pad="C18"/>
<connect gate="_" pin="IN2" pad="AN18"/>
<connect gate="_" pin="IN3" pad="AM18"/>
<connect gate="_" pin="MSEL0" pad="F5"/>
<connect gate="_" pin="MSEL1" pad="C1"/>
<connect gate="_" pin="TCK" pad="AL31"/>
<connect gate="_" pin="TDI" pad="AN1"/>
<connect gate="_" pin="TDO" pad="AN34"/>
<connect gate="_" pin="TMS" pad="C35"/>
<connect gate="_" pin="TRST" pad="C34"/>
<connect gate="_" pin="VCC_CKLK" pad="P5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K200EBC600-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8896"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K200-PGA599" prefix="IC">
<description>&lt;b&gt;EPF10K200&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="200P599C"/>
<gate name="-A" symbol="A11-599"/>
<gate name="-B" symbol="B11-599"/>
<gate name="-C" symbol="C10-599"/>
<gate name="-D" symbol="D11-599"/>
<gate name="-E" symbol="E11-599"/>
<gate name="-F" symbol="F10-599"/>
<gate name="-G" symbol="G11-599"/>
<gate name="-H" symbol="H11-599"/>
<gate name="-I" symbol="I11-599"/>
<gate name="-J" symbol="J12-599"/>
<gate name="-K" symbol="K11-599"/>
<gate name="-L" symbol="L10-599"/>
<gate name="-M" symbol="M11-599"/>
<gate name="-N" symbol="N11-599"/>
<gate name="-O" symbol="O10-599"/>
<gate name="-P" symbol="P11-599"/>
<gate name="-Q" symbol="Q11-599"/>
<gate name="-R" symbol="R10-599"/>
<gate name="-S" symbol="S11-599"/>
<gate name="-T" symbol="T11-599"/>
<gate name="-U" symbol="U10-599"/>
<gate name="-V" symbol="V11-599"/>
<gate name="-W" symbol="W11-599"/>
<gate name="-X" symbol="X10-599"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="-10" symbol="IO404"/>
<gate name="-11" symbol="IO444"/>
<gate name="-12" symbol="IO484"/>
<gate name="-13" symbol="IO524"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="G50" symbol="GND"/>
<gate name="G51" symbol="GND"/>
<gate name="G52" symbol="GND"/>
<gate name="G53" symbol="GND"/>
<gate name="G54" symbol="GND"/>
<gate name="G55" symbol="GND"/>
<gate name="G56" symbol="GND"/>
<gate name="G57" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="V24" symbol="VCCINT"/>
<gate name="V25" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
<gate name="VO30" symbol="VCCIO"/>
<gate name="VO31" symbol="VCCIO"/>
<gate name="VO32" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="PGA599">
<connects>
<connect gate="-1" pin="IO11" pad="C5"/>
<connect gate="-1" pin="IO12" pad="AY10"/>
<connect gate="-1" pin="IO13" pad="BD6"/>
<connect gate="-1" pin="IO14" pad="G9"/>
<connect gate="-1" pin="IO21" pad="B6"/>
<connect gate="-1" pin="IO22" pad="BA9"/>
<connect gate="-1" pin="IO23" pad="BF6"/>
<connect gate="-1" pin="IO24" pad="F8"/>
<connect gate="-1" pin="IO31" pad="D8"/>
<connect gate="-1" pin="IO32" pad="BB8"/>
<connect gate="-1" pin="IO33" pad="BD8"/>
<connect gate="-1" pin="IO34" pad="D6"/>
<connect gate="-1" pin="IO41" pad="C7"/>
<connect gate="-1" pin="IO42" pad="BA11"/>
<connect gate="-1" pin="IO43" pad="BE7"/>
<connect gate="-1" pin="IO44" pad="G11"/>
<connect gate="-10" pin="IO371" pad="BG33"/>
<connect gate="-10" pin="IO372" pad="BD32"/>
<connect gate="-10" pin="IO373" pad="B34"/>
<connect gate="-10" pin="IO374" pad="D32"/>
<connect gate="-10" pin="IO381" pad="A35"/>
<connect gate="-10" pin="IO382" pad="BE33"/>
<connect gate="-10" pin="IO383" pad="BD34"/>
<connect gate="-10" pin="IO384" pad="D34"/>
<connect gate="-10" pin="IO391" pad="B36"/>
<connect gate="-10" pin="IO392" pad="BA31"/>
<connect gate="-10" pin="IO393" pad="BF34"/>
<connect gate="-10" pin="IO394" pad="G31"/>
<connect gate="-10" pin="IO401" pad="BG35"/>
<connect gate="-10" pin="IO402" pad="A37"/>
<connect gate="-10" pin="IO403" pad="BB32"/>
<connect gate="-10" pin="IO404" pad="F32"/>
<connect gate="-11" pin="IO411" pad="A39"/>
<connect gate="-11" pin="IO412" pad="BD36"/>
<connect gate="-11" pin="IO413" pad="BF36"/>
<connect gate="-11" pin="IO414" pad="D36"/>
<connect gate="-11" pin="IO421" pad="F34"/>
<connect gate="-11" pin="IO422" pad="BB34"/>
<connect gate="-11" pin="IO423" pad="BG37"/>
<connect gate="-11" pin="IO424" pad="B38"/>
<connect gate="-11" pin="IO431" pad="A41"/>
<connect gate="-11" pin="IO432" pad="BA33"/>
<connect gate="-11" pin="IO433" pad="BG39"/>
<connect gate="-11" pin="IO434" pad="G33"/>
<connect gate="-11" pin="IO441" pad="D38"/>
<connect gate="-11" pin="IO442" pad="BD38"/>
<connect gate="-11" pin="IO443" pad="BF38"/>
<connect gate="-11" pin="IO444" pad="B40"/>
<connect gate="-12" pin="IO451" pad="G35"/>
<connect gate="-12" pin="IO452" pad="BB36"/>
<connect gate="-12" pin="IO453" pad="BG41"/>
<connect gate="-12" pin="IO454" pad="E37"/>
<connect gate="-12" pin="IO461" pad="C39"/>
<connect gate="-12" pin="IO462" pad="BF40"/>
<connect gate="-12" pin="IO463" pad="BA35"/>
<connect gate="-12" pin="IO464" pad="F36"/>
<connect gate="-12" pin="IO471" pad="A43"/>
<connect gate="-12" pin="IO472" pad="BE39"/>
<connect gate="-12" pin="IO473" pad="BC37"/>
<connect gate="-12" pin="IO474" pad="D40"/>
<connect gate="-12" pin="IO481" pad="B42"/>
<connect gate="-12" pin="IO482" pad="BG43"/>
<connect gate="-12" pin="IO483" pad="BB38"/>
<connect gate="-12" pin="IO484" pad="F38"/>
<connect gate="-13" pin="IO491" pad="D42"/>
<connect gate="-13" pin="IO492" pad="BA37"/>
<connect gate="-13" pin="IO493" pad="BE41"/>
<connect gate="-13" pin="IO494" pad="G37"/>
<connect gate="-13" pin="IO501" pad="BD40"/>
<connect gate="-13" pin="IO502" pad="BB40"/>
<connect gate="-13" pin="IO503" pad="C41"/>
<connect gate="-13" pin="IO504" pad="F40"/>
<connect gate="-13" pin="IO511" pad="G39"/>
<connect gate="-13" pin="IO512" pad="BA39"/>
<connect gate="-13" pin="IO513" pad="BF42"/>
<connect gate="-13" pin="IO514" pad="B44"/>
<connect gate="-13" pin="IO521" pad="H38"/>
<connect gate="-13" pin="IO522" pad="AY38"/>
<connect gate="-13" pin="IO523" pad="BD42"/>
<connect gate="-13" pin="IO524" pad="C43"/>
<connect gate="-2" pin="IO51" pad="F10"/>
<connect gate="-2" pin="IO52" pad="A5"/>
<connect gate="-2" pin="IO53" pad="BB10"/>
<connect gate="-2" pin="IO54" pad="BG5"/>
<connect gate="-2" pin="IO61" pad="E11"/>
<connect gate="-2" pin="IO62" pad="BC11"/>
<connect gate="-2" pin="IO63" pad="BE9"/>
<connect gate="-2" pin="IO64" pad="C9"/>
<connect gate="-2" pin="IO71" pad="G13"/>
<connect gate="-2" pin="IO72" pad="BA13"/>
<connect gate="-2" pin="IO73" pad="BF8"/>
<connect gate="-2" pin="IO74" pad="B8"/>
<connect gate="-2" pin="IO81" pad="F12"/>
<connect gate="-2" pin="IO82" pad="A7"/>
<connect gate="-2" pin="IO83" pad="BB12"/>
<connect gate="-2" pin="IO84" pad="BG7"/>
<connect gate="-3" pin="IO101" pad="A9"/>
<connect gate="-3" pin="IO102" pad="BG9"/>
<connect gate="-3" pin="IO103" pad="BA15"/>
<connect gate="-3" pin="IO104" pad="G15"/>
<connect gate="-3" pin="IO111" pad="A11"/>
<connect gate="-3" pin="IO112" pad="BG11"/>
<connect gate="-3" pin="IO113" pad="BB14"/>
<connect gate="-3" pin="IO114" pad="F14"/>
<connect gate="-3" pin="IO121" pad="B12"/>
<connect gate="-3" pin="IO122" pad="BD12"/>
<connect gate="-3" pin="IO123" pad="BF12"/>
<connect gate="-3" pin="IO124" pad="D12"/>
<connect gate="-3" pin="IO91" pad="B10"/>
<connect gate="-3" pin="IO92" pad="BF10"/>
<connect gate="-3" pin="IO93" pad="BD10"/>
<connect gate="-3" pin="IO94" pad="D10"/>
<connect gate="-4" pin="IO131" pad="A13"/>
<connect gate="-4" pin="IO132" pad="BB16"/>
<connect gate="-4" pin="IO133" pad="BG13"/>
<connect gate="-4" pin="IO134" pad="F16"/>
<connect gate="-4" pin="IO141" pad="B14"/>
<connect gate="-4" pin="IO142" pad="BA17"/>
<connect gate="-4" pin="IO143" pad="BF14"/>
<connect gate="-4" pin="IO144" pad="G17"/>
<connect gate="-4" pin="IO151" pad="C15"/>
<connect gate="-4" pin="IO152" pad="BD14"/>
<connect gate="-4" pin="IO153" pad="BE15"/>
<connect gate="-4" pin="IO154" pad="D14"/>
<connect gate="-4" pin="IO161" pad="A15"/>
<connect gate="-4" pin="IO162" pad="BD16"/>
<connect gate="-4" pin="IO163" pad="BG15"/>
<connect gate="-4" pin="IO164" pad="D16"/>
<connect gate="-5" pin="IO171" pad="B16"/>
<connect gate="-5" pin="IO172" pad="BF16"/>
<connect gate="-5" pin="IO173" pad="BB18"/>
<connect gate="-5" pin="IO174" pad="F18"/>
<connect gate="-5" pin="IO181" pad="C17"/>
<connect gate="-5" pin="IO182" pad="BE17"/>
<connect gate="-5" pin="IO183" pad="BA19"/>
<connect gate="-5" pin="IO184" pad="G19"/>
<connect gate="-5" pin="IO191" pad="A17"/>
<connect gate="-5" pin="IO192" pad="BG17"/>
<connect gate="-5" pin="IO193" pad="BC17"/>
<connect gate="-5" pin="IO194" pad="E17"/>
<connect gate="-5" pin="IO201" pad="B18"/>
<connect gate="-5" pin="IO202" pad="BF18"/>
<connect gate="-5" pin="IO203" pad="BD18"/>
<connect gate="-5" pin="IO204" pad="D18"/>
<connect gate="-6" pin="IO211" pad="F20"/>
<connect gate="-6" pin="IO212" pad="BG19"/>
<connect gate="-6" pin="IO213" pad="BB20"/>
<connect gate="-6" pin="IO214" pad="A19"/>
<connect gate="-6" pin="IO221" pad="G21"/>
<connect gate="-6" pin="IO222" pad="BF20"/>
<connect gate="-6" pin="IO223" pad="BA21"/>
<connect gate="-6" pin="IO224" pad="B20"/>
<connect gate="-6" pin="IO231" pad="D20"/>
<connect gate="-6" pin="IO232" pad="BG21"/>
<connect gate="-6" pin="IO233" pad="BD20"/>
<connect gate="-6" pin="IO234" pad="A21"/>
<connect gate="-6" pin="IO241" pad="D22"/>
<connect gate="-6" pin="IO242" pad="BF22"/>
<connect gate="-6" pin="IO243" pad="BB22"/>
<connect gate="-6" pin="IO244" pad="B22"/>
<connect gate="-7" pin="IO251" pad="BD22"/>
<connect gate="-7" pin="IO252" pad="BA23"/>
<connect gate="-7" pin="IO253" pad="C23"/>
<connect gate="-7" pin="IO254" pad="F22"/>
<connect gate="-7" pin="IO261" pad="BC23"/>
<connect gate="-7" pin="IO262" pad="BE23"/>
<connect gate="-7" pin="IO263" pad="A23"/>
<connect gate="-7" pin="IO264" pad="E23"/>
<connect gate="-7" pin="IO271" pad="E25"/>
<connect gate="-7" pin="IO272" pad="BC25"/>
<connect gate="-7" pin="IO273" pad="BE25"/>
<connect gate="-7" pin="IO274" pad="B26"/>
<connect gate="-7" pin="IO281" pad="F26"/>
<connect gate="-7" pin="IO282" pad="A27"/>
<connect gate="-7" pin="IO283" pad="BA25"/>
<connect gate="-7" pin="IO284" pad="BD26"/>
<connect gate="-8" pin="IO291" pad="B28"/>
<connect gate="-8" pin="IO292" pad="BB26"/>
<connect gate="-8" pin="IO293" pad="BF26"/>
<connect gate="-8" pin="IO294" pad="D26"/>
<connect gate="-8" pin="IO301" pad="A29"/>
<connect gate="-8" pin="IO302" pad="BG27"/>
<connect gate="-8" pin="IO303" pad="BD28"/>
<connect gate="-8" pin="IO304" pad="D28"/>
<connect gate="-8" pin="IO311" pad="B30"/>
<connect gate="-8" pin="IO312" pad="BF28"/>
<connect gate="-8" pin="IO313" pad="BA27"/>
<connect gate="-8" pin="IO314" pad="G27"/>
<connect gate="-8" pin="IO321" pad="A31"/>
<connect gate="-8" pin="IO322" pad="BG29"/>
<connect gate="-8" pin="IO323" pad="BB28"/>
<connect gate="-8" pin="IO324" pad="F28"/>
<connect gate="-9" pin="IO331" pad="D30"/>
<connect gate="-9" pin="IO332" pad="BD30"/>
<connect gate="-9" pin="IO333" pad="BF30"/>
<connect gate="-9" pin="IO334" pad="C31"/>
<connect gate="-9" pin="IO341" pad="E31"/>
<connect gate="-9" pin="IO342" pad="BC31"/>
<connect gate="-9" pin="IO343" pad="BG31"/>
<connect gate="-9" pin="IO344" pad="B32"/>
<connect gate="-9" pin="IO351" pad="G29"/>
<connect gate="-9" pin="IO352" pad="BA29"/>
<connect gate="-9" pin="IO353" pad="A33"/>
<connect gate="-9" pin="IO354" pad="BE31"/>
<connect gate="-9" pin="IO361" pad="C33"/>
<connect gate="-9" pin="IO362" pad="F30"/>
<connect gate="-9" pin="IO363" pad="BB30"/>
<connect gate="-9" pin="IO364" pad="BF32"/>
<connect gate="-A" pin="IOA1" pad="AW39"/>
<connect gate="-A" pin="IOA10" pad="BD4"/>
<connect gate="-A" pin="IOA11" pad="BF2"/>
<connect gate="-A" pin="IOA2" pad="BF46"/>
<connect gate="-A" pin="IOA3" pad="AY42"/>
<connect gate="-A" pin="IOA4" pad="AW9"/>
<connect gate="-A" pin="IOA5" pad="AY4"/>
<connect gate="-A" pin="IOA6" pad="AY6"/>
<connect gate="-A" pin="IOA7" pad="AY44"/>
<connect gate="-A" pin="IOA8" pad="BC3"/>
<connect gate="-A" pin="IOA9" pad="BC45"/>
<connect gate="-B" pin="IOB1" pad="BB44"/>
<connect gate="-B" pin="IOB10" pad="BD2"/>
<connect gate="-B" pin="IOB11" pad="BD46"/>
<connect gate="-B" pin="IOB2" pad="AW41"/>
<connect gate="-B" pin="IOB3" pad="AV8"/>
<connect gate="-B" pin="IOB4" pad="BB4"/>
<connect gate="-B" pin="IOB5" pad="AV6"/>
<connect gate="-B" pin="IOB6" pad="AV40"/>
<connect gate="-B" pin="IOB7" pad="AV42"/>
<connect gate="-B" pin="IOB8" pad="AW7"/>
<connect gate="-B" pin="IOB9" pad="BB46"/>
<connect gate="-C" pin="IOC1" pad="AV44"/>
<connect gate="-C" pin="IOC10" pad="BC47"/>
<connect gate="-C" pin="IOC2" pad="AT40"/>
<connect gate="-C" pin="IOC3" pad="AT8"/>
<connect gate="-C" pin="IOC4" pad="AV4"/>
<connect gate="-C" pin="IOC5" pad="AU7"/>
<connect gate="-C" pin="IOC6" pad="AU41"/>
<connect gate="-C" pin="IOC7" pad="BA3"/>
<connect gate="-C" pin="IOC8" pad="BA45"/>
<connect gate="-C" pin="IOC9" pad="BB2"/>
<connect gate="-D" pin="IOD1" pad="AW45"/>
<connect gate="-D" pin="IOD10" pad="AY46"/>
<connect gate="-D" pin="IOD11" pad="BC1"/>
<connect gate="-D" pin="IOD2" pad="AT44"/>
<connect gate="-D" pin="IOD3" pad="AT4"/>
<connect gate="-D" pin="IOD4" pad="AY2"/>
<connect gate="-D" pin="IOD5" pad="AT6"/>
<connect gate="-D" pin="IOD6" pad="AT42"/>
<connect gate="-D" pin="IOD7" pad="AU5"/>
<connect gate="-D" pin="IOD8" pad="AU43"/>
<connect gate="-D" pin="IOD9" pad="AW3"/>
<connect gate="-E" pin="IOE1" pad="AP42"/>
<connect gate="-E" pin="IOE10" pad="AW47"/>
<connect gate="-E" pin="IOE11" pad="BA47"/>
<connect gate="-E" pin="IOE2" pad="BA1"/>
<connect gate="-E" pin="IOE3" pad="AP4"/>
<connect gate="-E" pin="IOE4" pad="AP6"/>
<connect gate="-E" pin="IOE5" pad="AP8"/>
<connect gate="-E" pin="IOE6" pad="AP40"/>
<connect gate="-E" pin="IOE7" pad="AP44"/>
<connect gate="-E" pin="IOE8" pad="AR7"/>
<connect gate="-E" pin="IOE9" pad="AR41"/>
<connect gate="-F" pin="IOF1" pad="AN41"/>
<connect gate="-F" pin="IOF10" pad="AW1"/>
<connect gate="-F" pin="IOF2" pad="AU47"/>
<connect gate="-F" pin="IOF3" pad="AM8"/>
<connect gate="-F" pin="IOF4" pad="AM40"/>
<connect gate="-F" pin="IOF5" pad="AN7"/>
<connect gate="-F" pin="IOF6" pad="AT46"/>
<connect gate="-F" pin="IOF7" pad="AU1"/>
<connect gate="-F" pin="IOF8" pad="AV2"/>
<connect gate="-F" pin="IOF9" pad="AV46"/>
<connect gate="-G" pin="IOG1" pad="AM44"/>
<connect gate="-G" pin="IOG10" pad="AR47"/>
<connect gate="-G" pin="IOG11" pad="AT2"/>
<connect gate="-G" pin="IOG2" pad="AM4"/>
<connect gate="-G" pin="IOG3" pad="AL7"/>
<connect gate="-G" pin="IOG4" pad="AL41"/>
<connect gate="-G" pin="IOG5" pad="AM6"/>
<connect gate="-G" pin="IOG6" pad="AM42"/>
<connect gate="-G" pin="IOG7" pad="AP2"/>
<connect gate="-G" pin="IOG8" pad="AP46"/>
<connect gate="-G" pin="IOG9" pad="AR1"/>
<connect gate="-H" pin="IOH1" pad="AK6"/>
<connect gate="-H" pin="IOH10" pad="AN45"/>
<connect gate="-H" pin="IOH11" pad="AN47"/>
<connect gate="-H" pin="IOH2" pad="AK8"/>
<connect gate="-H" pin="IOH3" pad="AL5"/>
<connect gate="-H" pin="IOH4" pad="AK4"/>
<connect gate="-H" pin="IOH5" pad="AK40"/>
<connect gate="-H" pin="IOH6" pad="AK42"/>
<connect gate="-H" pin="IOH7" pad="AK44"/>
<connect gate="-H" pin="IOH8" pad="AL43"/>
<connect gate="-H" pin="IOH9" pad="AN3"/>
<connect gate="-I" pin="IOI10" pad="AM46"/>
<connect gate="-I" pin="IOI11" pad="AN1"/>
<connect gate="-I" pin="IOI2" pad="AJ41"/>
<connect gate="-I" pin="IOI3" pad="AH8"/>
<connect gate="-I" pin="IOI4" pad="AH40"/>
<connect gate="-I" pin="IOI5" pad="AJ7"/>
<connect gate="-I" pin="IOI6" pad="AL3"/>
<connect gate="-I" pin="IOI7" pad="AL45"/>
<connect gate="-I" pin="IOI8" pad="AL47"/>
<connect gate="-I" pin="IOI9" pad="AM2"/>
<connect gate="-J" pin="IOJ1" pad="AH42"/>
<connect gate="-J" pin="IOJ10" pad="AJ47"/>
<connect gate="-J" pin="IOJ11" pad="AK46"/>
<connect gate="-J" pin="IOJ12" pad="AL1"/>
<connect gate="-J" pin="IOJ3" pad="AH4"/>
<connect gate="-J" pin="IOJ4" pad="AK2"/>
<connect gate="-J" pin="IOJ5" pad="AG7"/>
<connect gate="-J" pin="IOJ6" pad="AG41"/>
<connect gate="-J" pin="IOJ7" pad="AH6"/>
<connect gate="-J" pin="IOJ8" pad="AH44"/>
<connect gate="-J" pin="IOJ9" pad="AJ1"/>
<connect gate="-K" pin="IOK1" pad="AG47"/>
<connect gate="-K" pin="IOK10" pad="AH2"/>
<connect gate="-K" pin="IOK11" pad="AH46"/>
<connect gate="-K" pin="IOK2" pad="AF42"/>
<connect gate="-K" pin="IOK3" pad="AF4"/>
<connect gate="-K" pin="IOK4" pad="AG1"/>
<connect gate="-K" pin="IOK5" pad="AF6"/>
<connect gate="-K" pin="IOK6" pad="AF8"/>
<connect gate="-K" pin="IOK7" pad="AF40"/>
<connect gate="-K" pin="IOK8" pad="AF44"/>
<connect gate="-K" pin="IOK9" pad="AF46"/>
<connect gate="-L" pin="IOL1" pad="AE47"/>
<connect gate="-L" pin="IOL10" pad="AF2"/>
<connect gate="-L" pin="IOL2" pad="AE43"/>
<connect gate="-L" pin="IOL3" pad="AE1"/>
<connect gate="-L" pin="IOL4" pad="AD46"/>
<connect gate="-L" pin="IOL5" pad="AE3"/>
<connect gate="-L" pin="IOL6" pad="AE5"/>
<connect gate="-L" pin="IOL7" pad="AE7"/>
<connect gate="-L" pin="IOL8" pad="AE41"/>
<connect gate="-L" pin="IOL9" pad="AE45"/>
<connect gate="-M" pin="IOM1" pad="AC45"/>
<connect gate="-M" pin="IOM10" pad="AD8"/>
<connect gate="-M" pin="IOM11" pad="AD40"/>
<connect gate="-M" pin="IOM2" pad="AC43"/>
<connect gate="-M" pin="IOM3" pad="AC3"/>
<connect gate="-M" pin="IOM4" pad="AC1"/>
<connect gate="-M" pin="IOM5" pad="AC5"/>
<connect gate="-M" pin="IOM6" pad="AC7"/>
<connect gate="-M" pin="IOM7" pad="AC41"/>
<connect gate="-M" pin="IOM8" pad="AC47"/>
<connect gate="-M" pin="IOM9" pad="AD2"/>
<connect gate="-N" pin="ION1" pad="AB44"/>
<connect gate="-N" pin="ION10" pad="AB46"/>
<connect gate="-N" pin="ION11" pad="Y46"/>
<connect gate="-N" pin="ION2" pad="AB40"/>
<connect gate="-N" pin="ION3" pad="AB8"/>
<connect gate="-N" pin="ION4" pad="AB2"/>
<connect gate="-N" pin="ION5" pad="AA1"/>
<connect gate="-N" pin="ION6" pad="AA47"/>
<connect gate="-N" pin="ION7" pad="AB4"/>
<connect gate="-N" pin="ION8" pad="AB6"/>
<connect gate="-N" pin="ION9" pad="AB42"/>
<connect gate="-O" pin="IOO1" pad="AA41"/>
<connect gate="-O" pin="IOO10" pad="Y44"/>
<connect gate="-O" pin="IOO2" pad="Y4"/>
<connect gate="-O" pin="IOO3" pad="W1"/>
<connect gate="-O" pin="IOO4" pad="AA7"/>
<connect gate="-O" pin="IOO5" pad="U47"/>
<connect gate="-O" pin="IOO6" pad="V2"/>
<connect gate="-O" pin="IOO7" pad="V46"/>
<connect gate="-O" pin="IOO8" pad="W47"/>
<connect gate="-O" pin="IOO9" pad="Y2"/>
<connect gate="-P" pin="IOP1" pad="U45"/>
<connect gate="-P" pin="IOP10" pad="Y40"/>
<connect gate="-P" pin="IOP11" pad="Y42"/>
<connect gate="-P" pin="IOP2" pad="U3"/>
<connect gate="-P" pin="IOP3" pad="Y6"/>
<connect gate="-P" pin="IOP4" pad="T2"/>
<connect gate="-P" pin="IOP5" pad="T46"/>
<connect gate="-P" pin="IOP6" pad="U1"/>
<connect gate="-P" pin="IOP7" pad="W7"/>
<connect gate="-P" pin="IOP8" pad="W41"/>
<connect gate="-P" pin="IOP9" pad="Y8"/>
<connect gate="-Q" pin="IOQ1" pad="V42"/>
<connect gate="-Q" pin="IOQ10" pad="V40"/>
<connect gate="-Q" pin="IOQ11" pad="V44"/>
<connect gate="-Q" pin="IOQ2" pad="R1"/>
<connect gate="-Q" pin="IOQ3" pad="V6"/>
<connect gate="-Q" pin="IOQ4" pad="R45"/>
<connect gate="-Q" pin="IOQ5" pad="R47"/>
<connect gate="-Q" pin="IOQ6" pad="U5"/>
<connect gate="-Q" pin="IOQ7" pad="U43"/>
<connect gate="-Q" pin="IOQ8" pad="V4"/>
<connect gate="-Q" pin="IOQ9" pad="V8"/>
<connect gate="-R" pin="IOR1" pad="N47"/>
<connect gate="-R" pin="IOR10" pad="U41"/>
<connect gate="-R" pin="IOR2" pad="T44"/>
<connect gate="-R" pin="IOR3" pad="M46"/>
<connect gate="-R" pin="IOR4" pad="N1"/>
<connect gate="-R" pin="IOR5" pad="P2"/>
<connect gate="-R" pin="IOR6" pad="P46"/>
<connect gate="-R" pin="IOR7" pad="R3"/>
<connect gate="-R" pin="IOR8" pad="T4"/>
<connect gate="-R" pin="IOR9" pad="U7"/>
<connect gate="-S" pin="IOS1" pad="K46"/>
<connect gate="-S" pin="IOS10" pad="T40"/>
<connect gate="-S" pin="IOS11" pad="T42"/>
<connect gate="-S" pin="IOS2" pad="R41"/>
<connect gate="-S" pin="IOS3" pad="T8"/>
<connect gate="-S" pin="IOS4" pad="K2"/>
<connect gate="-S" pin="IOS5" pad="L1"/>
<connect gate="-S" pin="IOS6" pad="L47"/>
<connect gate="-S" pin="IOS7" pad="M2"/>
<connect gate="-S" pin="IOS8" pad="R7"/>
<connect gate="-S" pin="IOS9" pad="T6"/>
<connect gate="-T" pin="IOT1" pad="P42"/>
<connect gate="-T" pin="IOT10" pad="P40"/>
<connect gate="-T" pin="IOT11" pad="P44"/>
<connect gate="-T" pin="IOT2" pad="P6"/>
<connect gate="-T" pin="IOT3" pad="P8"/>
<connect gate="-T" pin="IOT4" pad="J1"/>
<connect gate="-T" pin="IOT5" pad="J45"/>
<connect gate="-T" pin="IOT6" pad="J47"/>
<connect gate="-T" pin="IOT7" pad="N7"/>
<connect gate="-T" pin="IOT8" pad="N41"/>
<connect gate="-T" pin="IOT9" pad="P4"/>
<connect gate="-U" pin="IOU1" pad="G47"/>
<connect gate="-U" pin="IOU10" pad="M44"/>
<connect gate="-U" pin="IOU2" pad="M42"/>
<connect gate="-U" pin="IOU3" pad="H2"/>
<connect gate="-U" pin="IOU4" pad="M4"/>
<connect gate="-U" pin="IOU5" pad="G1"/>
<connect gate="-U" pin="IOU6" pad="H46"/>
<connect gate="-U" pin="IOU7" pad="J3"/>
<connect gate="-U" pin="IOU8" pad="M6"/>
<connect gate="-U" pin="IOU9" pad="K40"/>
<connect gate="-V" pin="IOV1" pad="L41"/>
<connect gate="-V" pin="IOV10" pad="L43"/>
<connect gate="-V" pin="IOV11" pad="M8"/>
<connect gate="-V" pin="IOV2" pad="G45"/>
<connect gate="-V" pin="IOV3" pad="H4"/>
<connect gate="-V" pin="IOV4" pad="L7"/>
<connect gate="-V" pin="IOV5" pad="G3"/>
<connect gate="-V" pin="IOV6" pad="H44"/>
<connect gate="-V" pin="IOV7" pad="K4"/>
<connect gate="-V" pin="IOV8" pad="K44"/>
<connect gate="-V" pin="IOV9" pad="L5"/>
<connect gate="-W" pin="IOW1" pad="F46"/>
<connect gate="-W" pin="IOW10" pad="M40"/>
<connect gate="-W" pin="IOW11" pad="K42"/>
<connect gate="-W" pin="IOW2" pad="F4"/>
<connect gate="-W" pin="IOW3" pad="K8"/>
<connect gate="-W" pin="IOW4" pad="E47"/>
<connect gate="-W" pin="IOW5" pad="F2"/>
<connect gate="-W" pin="IOW6" pad="F44"/>
<connect gate="-W" pin="IOW7" pad="J7"/>
<connect gate="-W" pin="IOW8" pad="J41"/>
<connect gate="-W" pin="IOW9" pad="K6"/>
<connect gate="-X" pin="IOX1" pad="E45"/>
<connect gate="-X" pin="IOX10" pad="J39"/>
<connect gate="-X" pin="IOX2" pad="H42"/>
<connect gate="-X" pin="IOX3" pad="H8"/>
<connect gate="-X" pin="IOX4" pad="E3"/>
<connect gate="-X" pin="IOX5" pad="D2"/>
<connect gate="-X" pin="IOX6" pad="D44"/>
<connect gate="-X" pin="IOX7" pad="D46"/>
<connect gate="-X" pin="IOX8" pad="E1"/>
<connect gate="-X" pin="IOX9" pad="H6"/>
<connect gate="G1" pin="GND" pad="AA3"/>
<connect gate="G10" pin="GND" pad="AR5"/>
<connect gate="G11" pin="GND" pad="AR43"/>
<connect gate="G12" pin="GND" pad="AR45"/>
<connect gate="G13" pin="GND" pad="AY8"/>
<connect gate="G14" pin="GND" pad="AY40"/>
<connect gate="G15" pin="GND" pad="A47"/>
<connect gate="G16" pin="GND" pad="BA5"/>
<connect gate="G17" pin="GND" pad="BA43"/>
<connect gate="G18" pin="GND" pad="BB24"/>
<connect gate="G19" pin="GND" pad="BC7"/>
<connect gate="G2" pin="GND" pad="AA45"/>
<connect gate="G20" pin="GND" pad="BC13"/>
<connect gate="G21" pin="GND" pad="BC19"/>
<connect gate="G22" pin="GND" pad="BC29"/>
<connect gate="G23" pin="GND" pad="BC35"/>
<connect gate="G24" pin="GND" pad="BC41"/>
<connect gate="G25" pin="GND" pad="BD44"/>
<connect gate="G26" pin="GND" pad="BE3"/>
<connect gate="G27" pin="GND" pad="BE13"/>
<connect gate="G28" pin="GND" pad="BE21"/>
<connect gate="G29" pin="GND" pad="BE27"/>
<connect gate="G3" pin="GND" pad="AD6"/>
<connect gate="G30" pin="GND" pad="BE35"/>
<connect gate="G31" pin="GND" pad="BE45"/>
<connect gate="G32" pin="GND" pad="BG1"/>
<connect gate="G33" pin="GND" pad="BG47"/>
<connect gate="G34" pin="GND" pad="B2"/>
<connect gate="G35" pin="GND" pad="C13"/>
<connect gate="G36" pin="GND" pad="C21"/>
<connect gate="G37" pin="GND" pad="C27"/>
<connect gate="G38" pin="GND" pad="C35"/>
<connect gate="G39" pin="GND" pad="C45"/>
<connect gate="G4" pin="GND" pad="AD42"/>
<connect gate="G40" pin="GND" pad="D4"/>
<connect gate="G41" pin="GND" pad="E7"/>
<connect gate="G42" pin="GND" pad="E13"/>
<connect gate="G43" pin="GND" pad="E19"/>
<connect gate="G44" pin="GND" pad="E29"/>
<connect gate="G45" pin="GND" pad="E35"/>
<connect gate="G46" pin="GND" pad="E41"/>
<connect gate="G47" pin="GND" pad="F24"/>
<connect gate="G48" pin="GND" pad="G5"/>
<connect gate="G49" pin="GND" pad="G23"/>
<connect gate="G5" pin="GND" pad="AG3"/>
<connect gate="G50" pin="GND" pad="G43"/>
<connect gate="G51" pin="GND" pad="H40"/>
<connect gate="G52" pin="GND" pad="N3"/>
<connect gate="G53" pin="GND" pad="N5"/>
<connect gate="G54" pin="GND" pad="N43"/>
<connect gate="G55" pin="GND" pad="N45"/>
<connect gate="G56" pin="GND" pad="W5"/>
<connect gate="G57" pin="GND" pad="W43"/>
<connect gate="G6" pin="GND" pad="AG45"/>
<connect gate="G7" pin="GND" pad="AJ5"/>
<connect gate="G8" pin="GND" pad="AJ43"/>
<connect gate="G9" pin="GND" pad="AR3"/>
<connect gate="V1" pin="VCC" pad="AJ3"/>
<connect gate="V10" pin="VCC" pad="BE29"/>
<connect gate="V11" pin="VCC" pad="BE37"/>
<connect gate="V12" pin="VCC" pad="BE47"/>
<connect gate="V13" pin="VCC" pad="BG3"/>
<connect gate="V14" pin="VCC" pad="BG45"/>
<connect gate="V15" pin="VCC" pad="C1"/>
<connect gate="V16" pin="VCC" pad="C11"/>
<connect gate="V17" pin="VCC" pad="C19"/>
<connect gate="V18" pin="VCC" pad="C29"/>
<connect gate="V19" pin="VCC" pad="C37"/>
<connect gate="V2" pin="VCC" pad="AJ45"/>
<connect gate="V20" pin="VCC" pad="C47"/>
<connect gate="V21" pin="VCC" pad="E5"/>
<connect gate="V22" pin="VCC" pad="G25"/>
<connect gate="V23" pin="VCC" pad="L3"/>
<connect gate="V24" pin="VCC" pad="L45"/>
<connect gate="V25" pin="VCC" pad="W45"/>
<connect gate="V3" pin="VCC" pad="AU3"/>
<connect gate="V4" pin="VCC" pad="AU45"/>
<connect gate="V5" pin="VCC" pad="A3"/>
<connect gate="V6" pin="VCC" pad="A45"/>
<connect gate="V7" pin="VCC" pad="BE1"/>
<connect gate="V8" pin="VCC" pad="BE11"/>
<connect gate="V9" pin="VCC" pad="BE19"/>
<connect gate="VO1" pin="VCCIO" pad="AA5"/>
<connect gate="VO10" pin="VCCIO" pad="AW43"/>
<connect gate="VO11" pin="VCCIO" pad="BA7"/>
<connect gate="VO12" pin="VCCIO" pad="BA41"/>
<connect gate="VO13" pin="VCCIO" pad="BC9"/>
<connect gate="VO14" pin="VCCIO" pad="BC15"/>
<connect gate="VO15" pin="VCCIO" pad="BC21"/>
<connect gate="VO16" pin="VCCIO" pad="BC27"/>
<connect gate="VO17" pin="VCCIO" pad="BC33"/>
<connect gate="VO18" pin="VCCIO" pad="BC39"/>
<connect gate="VO19" pin="VCCIO" pad="BD24"/>
<connect gate="VO2" pin="VCCIO" pad="AA43"/>
<connect gate="VO20" pin="VCCIO" pad="D24"/>
<connect gate="VO21" pin="VCCIO" pad="E9"/>
<connect gate="VO22" pin="VCCIO" pad="E15"/>
<connect gate="VO23" pin="VCCIO" pad="E21"/>
<connect gate="VO24" pin="VCCIO" pad="E27"/>
<connect gate="VO25" pin="VCCIO" pad="E33"/>
<connect gate="VO26" pin="VCCIO" pad="E39"/>
<connect gate="VO27" pin="VCCIO" pad="G7"/>
<connect gate="VO28" pin="VCCIO" pad="G41"/>
<connect gate="VO29" pin="VCCIO" pad="J5"/>
<connect gate="VO3" pin="VCCIO" pad="AD4"/>
<connect gate="VO30" pin="VCCIO" pad="J43"/>
<connect gate="VO31" pin="VCCIO" pad="R5"/>
<connect gate="VO32" pin="VCCIO" pad="R43"/>
<connect gate="VO4" pin="VCCIO" pad="AD44"/>
<connect gate="VO5" pin="VCCIO" pad="AG5"/>
<connect gate="VO6" pin="VCCIO" pad="AG43"/>
<connect gate="VO7" pin="VCCIO" pad="AN5"/>
<connect gate="VO8" pin="VCCIO" pad="AN43"/>
<connect gate="VO9" pin="VCCIO" pad="AW5"/>
<connect gate="_" pin="/CE" pad="BB6"/>
<connect gate="_" pin="/CEO" pad="BF44"/>
<connect gate="_" pin="/CONFIG" pad="B4"/>
<connect gate="_" pin="/STATUS" pad="E43"/>
<connect gate="_" pin="CONF_DONE" pad="BC43"/>
<connect gate="_" pin="DATA0" pad="BC5"/>
<connect gate="_" pin="DCLK" pad="BE5"/>
<connect gate="_" pin="GCLK" pad="BF24"/>
<connect gate="_" pin="GCLK1" pad="A25"/>
<connect gate="_" pin="IN0" pad="C25"/>
<connect gate="_" pin="IN1" pad="B24"/>
<connect gate="_" pin="IN2" pad="BG23"/>
<connect gate="_" pin="IN3" pad="BG25"/>
<connect gate="_" pin="MSEL0" pad="F6"/>
<connect gate="_" pin="MSEL1" pad="C3"/>
<connect gate="_" pin="TCK" pad="BE43"/>
<connect gate="_" pin="TDI" pad="BF4"/>
<connect gate="_" pin="TDO" pad="BB42"/>
<connect gate="_" pin="TMS" pad="F42"/>
<connect gate="_" pin="TRST" pad="B46"/>
<connect gate="_" pin="VCC_CKLK" pad="W3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K200-RQ240" prefix="IC">
<description>&lt;b&gt;EPF10K200&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="R240C"/>
<gate name="-A" symbol="A4-D4"/>
<gate name="-B" symbol="E2-J4"/>
<gate name="-C" symbol="K4-O3"/>
<gate name="-D" symbol="P3-T3"/>
<gate name="-E" symbol="U4-X4"/>
<gate name="-1" symbol="122-200"/>
<gate name="-2" symbol="201-200"/>
<gate name="-3" symbol="261-200"/>
<gate name="-4" symbol="351-200"/>
<gate name="-5" symbol="441-200"/>
<gate name="-6" symbol="522-200"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="VI1" symbol="VCCINT"/>
<gate name="VI2" symbol="VCCINT"/>
<gate name="VI3" symbol="VCCINT"/>
<gate name="VI4" symbol="VCCINT"/>
<gate name="VI5" symbol="VCCINT"/>
<gate name="VI6" symbol="VCCINT"/>
<gate name="VI7" symbol="VCCINT"/>
<gate name="VI8" symbol="VCCINT"/>
<gate name="VI9" symbol="VCCINT"/>
<gate name="VI10" symbol="VCCINT"/>
<gate name="VI11" symbol="VCCINT"/>
<gate name="VI12" symbol="VCCINT"/>
<gate name="VI13" symbol="VCCINT"/>
<gate name="VI14" symbol="VCCINT"/>
<gate name="VI15" symbol="VCCINT"/>
<gate name="VI16" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="RQFP240">
<connects>
<connect gate="-1" pin="IO101" pad="110"/>
<connect gate="-1" pin="IO102" pad="182"/>
<connect gate="-1" pin="IO11" pad="120"/>
<connect gate="-1" pin="IO111" pad="109"/>
<connect gate="-1" pin="IO112" pad="183"/>
<connect gate="-1" pin="IO121" pad="108"/>
<connect gate="-1" pin="IO122" pad="184"/>
<connect gate="-1" pin="IO21" pad="119"/>
<connect gate="-1" pin="IO31" pad="118"/>
<connect gate="-1" pin="IO41" pad="117"/>
<connect gate="-1" pin="IO51" pad="116"/>
<connect gate="-1" pin="IO61" pad="115"/>
<connect gate="-1" pin="IO71" pad="114"/>
<connect gate="-1" pin="IO81" pad="113"/>
<connect gate="-1" pin="IO91" pad="111"/>
<connect gate="-1" pin="IO92" pad="181"/>
<connect gate="-2" pin="IO123" pad="185"/>
<connect gate="-2" pin="IO131" pad="107"/>
<connect gate="-2" pin="IO132" pad="186"/>
<connect gate="-2" pin="IO141" pad="106"/>
<connect gate="-2" pin="IO142" pad="188"/>
<connect gate="-2" pin="IO151" pad="105"/>
<connect gate="-2" pin="IO152" pad="190"/>
<connect gate="-2" pin="IO161" pad="103"/>
<connect gate="-2" pin="IO162" pad="191"/>
<connect gate="-2" pin="IO171" pad="102"/>
<connect gate="-2" pin="IO172" pad="192"/>
<connect gate="-2" pin="IO181" pad="101"/>
<connect gate="-2" pin="IO182" pad="193"/>
<connect gate="-2" pin="IO191" pad="100"/>
<connect gate="-2" pin="IO192" pad="194"/>
<connect gate="-2" pin="IO201" pad="99"/>
<connect gate="-3" pin="IO202" pad="195"/>
<connect gate="-3" pin="IO211" pad="98"/>
<connect gate="-3" pin="IO212" pad="196"/>
<connect gate="-3" pin="IO213" pad="198"/>
<connect gate="-3" pin="IO221" pad="97"/>
<connect gate="-3" pin="IO222" pad="199"/>
<connect gate="-3" pin="IO223" pad="200"/>
<connect gate="-3" pin="IO231" pad="95"/>
<connect gate="-3" pin="IO232" pad="201"/>
<connect gate="-3" pin="IO233" pad="202"/>
<connect gate="-3" pin="IO241" pad="94"/>
<connect gate="-3" pin="IO242" pad="203"/>
<connect gate="-3" pin="IO243" pad="204"/>
<connect gate="-3" pin="IO251" pad="206"/>
<connect gate="-3" pin="IO252" pad="207"/>
<connect gate="-3" pin="IO261" pad="208"/>
<connect gate="-4" pin="IO262" pad="209"/>
<connect gate="-4" pin="IO271" pad="88"/>
<connect gate="-4" pin="IO272" pad="213"/>
<connect gate="-4" pin="IO281" pad="87"/>
<connect gate="-4" pin="IO291" pad="86"/>
<connect gate="-4" pin="IO301" pad="84"/>
<connect gate="-4" pin="IO302" pad="214"/>
<connect gate="-4" pin="IO311" pad="83"/>
<connect gate="-4" pin="IO312" pad="215"/>
<connect gate="-4" pin="IO321" pad="82"/>
<connect gate="-4" pin="IO322" pad="217"/>
<connect gate="-4" pin="IO331" pad="81"/>
<connect gate="-4" pin="IO332" pad="218"/>
<connect gate="-4" pin="IO341" pad="80"/>
<connect gate="-4" pin="IO342" pad="219"/>
<connect gate="-4" pin="IO351" pad="79"/>
<connect gate="-5" pin="IO352" pad="220"/>
<connect gate="-5" pin="IO361" pad="73"/>
<connect gate="-5" pin="IO362" pad="78"/>
<connect gate="-5" pin="IO363" pad="221"/>
<connect gate="-5" pin="IO371" pad="222"/>
<connect gate="-5" pin="IO381" pad="75"/>
<connect gate="-5" pin="IO382" pad="223"/>
<connect gate="-5" pin="IO391" pad="74"/>
<connect gate="-5" pin="IO401" pad="226"/>
<connect gate="-5" pin="IO411" pad="72"/>
<connect gate="-5" pin="IO412" pad="227"/>
<connect gate="-5" pin="IO421" pad="71"/>
<connect gate="-5" pin="IO422" pad="228"/>
<connect gate="-5" pin="IO431" pad="70"/>
<connect gate="-5" pin="IO432" pad="229"/>
<connect gate="-5" pin="IO441" pad="68"/>
<connect gate="-6" pin="IO442" pad="230"/>
<connect gate="-6" pin="IO451" pad="67"/>
<connect gate="-6" pin="IO452" pad="231"/>
<connect gate="-6" pin="IO461" pad="66"/>
<connect gate="-6" pin="IO462" pad="233"/>
<connect gate="-6" pin="IO471" pad="65"/>
<connect gate="-6" pin="IO472" pad="234"/>
<connect gate="-6" pin="IO481" pad="64"/>
<connect gate="-6" pin="IO482" pad="235"/>
<connect gate="-6" pin="IO491" pad="63"/>
<connect gate="-6" pin="IO492" pad="236"/>
<connect gate="-6" pin="IO501" pad="237"/>
<connect gate="-6" pin="IO502" pad="238"/>
<connect gate="-6" pin="IO511" pad="62"/>
<connect gate="-6" pin="IO512" pad="239"/>
<connect gate="-6" pin="IO521" pad="61"/>
<connect gate="-6" pin="IO522" pad="240"/>
<connect gate="-A" pin="IOA1" pad="6"/>
<connect gate="-A" pin="IOA2" pad="7"/>
<connect gate="-A" pin="IOA3" pad="11"/>
<connect gate="-A" pin="IOA4" pad="175"/>
<connect gate="-A" pin="IOB1" pad="8"/>
<connect gate="-A" pin="IOB2" pad="9"/>
<connect gate="-A" pin="IOB3" pad="173"/>
<connect gate="-A" pin="IOB4" pad="174"/>
<connect gate="-A" pin="IOC1" pad="12"/>
<connect gate="-A" pin="IOC2" pad="13"/>
<connect gate="-A" pin="IOC3" pad="171"/>
<connect gate="-A" pin="IOC4" pad="172"/>
<connect gate="-A" pin="IOD1" pad="14"/>
<connect gate="-A" pin="IOD2" pad="15"/>
<connect gate="-A" pin="IOD3" pad="168"/>
<connect gate="-A" pin="IOD4" pad="169"/>
<connect gate="-B" pin="IOE1" pad="17"/>
<connect gate="-B" pin="IOE2" pad="167"/>
<connect gate="-B" pin="IOF1" pad="18"/>
<connect gate="-B" pin="IOF2" pad="19"/>
<connect gate="-B" pin="IOF3" pad="166"/>
<connect gate="-B" pin="IOG1" pad="21"/>
<connect gate="-B" pin="IOG2" pad="164"/>
<connect gate="-B" pin="IOH1" pad="161"/>
<connect gate="-B" pin="IOH2" pad="162"/>
<connect gate="-B" pin="IOH3" pad="163"/>
<connect gate="-B" pin="IOI1" pad="23"/>
<connect gate="-B" pin="IOI2" pad="24"/>
<connect gate="-B" pin="IOI3" pad="158"/>
<connect gate="-B" pin="IOJ1" pad="25"/>
<connect gate="-B" pin="IOJ2" pad="26"/>
<connect gate="-B" pin="IOJ3" pad="156"/>
<connect gate="-B" pin="IOJ4" pad="157"/>
<connect gate="-C" pin="IOK1" pad="28"/>
<connect gate="-C" pin="IOK2" pad="29"/>
<connect gate="-C" pin="IOK3" pad="153"/>
<connect gate="-C" pin="IOK4" pad="154"/>
<connect gate="-C" pin="IOL1" pad="30"/>
<connect gate="-C" pin="IOL2" pad="31"/>
<connect gate="-C" pin="IOL3" pad="152"/>
<connect gate="-C" pin="IOM1" pad="33"/>
<connect gate="-C" pin="IOM2" pad="34"/>
<connect gate="-C" pin="IOM3" pad="151"/>
<connect gate="-C" pin="ION1" pad="35"/>
<connect gate="-C" pin="ION2" pad="36"/>
<connect gate="-C" pin="ION3" pad="148"/>
<connect gate="-C" pin="ION4" pad="149"/>
<connect gate="-C" pin="IOO1" pad="38"/>
<connect gate="-C" pin="IOO2" pad="146"/>
<connect gate="-C" pin="IOO3" pad="147"/>
<connect gate="-D" pin="IOP1" pad="39"/>
<connect gate="-D" pin="IOP2" pad="143"/>
<connect gate="-D" pin="IOP3" pad="144"/>
<connect gate="-D" pin="IOQ1" pad="41"/>
<connect gate="-D" pin="IOQ2" pad="141"/>
<connect gate="-D" pin="IOQ3" pad="142"/>
<connect gate="-D" pin="IOR1" pad="43"/>
<connect gate="-D" pin="IOR2" pad="44"/>
<connect gate="-D" pin="IOS1" pad="45"/>
<connect gate="-D" pin="IOS2" pad="46"/>
<connect gate="-D" pin="IOS3" pad="138"/>
<connect gate="-D" pin="IOT1" pad="48"/>
<connect gate="-D" pin="IOT2" pad="136"/>
<connect gate="-D" pin="IOT3" pad="137"/>
<connect gate="-E" pin="IOU1" pad="49"/>
<connect gate="-E" pin="IOU2" pad="50"/>
<connect gate="-E" pin="IOU3" pad="133"/>
<connect gate="-E" pin="IOU4" pad="134"/>
<connect gate="-E" pin="IOV1" pad="51"/>
<connect gate="-E" pin="IOV2" pad="53"/>
<connect gate="-E" pin="IOV3" pad="131"/>
<connect gate="-E" pin="IOV4" pad="132"/>
<connect gate="-E" pin="IOW1" pad="54"/>
<connect gate="-E" pin="IOW2" pad="128"/>
<connect gate="-E" pin="IOW3" pad="129"/>
<connect gate="-E" pin="IOX1" pad="55"/>
<connect gate="-E" pin="IOX2" pad="56"/>
<connect gate="-E" pin="IOX3" pad="126"/>
<connect gate="-E" pin="IOX4" pad="127"/>
<connect gate="G1" pin="GND" pad="10"/>
<connect gate="G10" pin="GND" pad="125"/>
<connect gate="G11" pin="GND" pad="135"/>
<connect gate="G12" pin="GND" pad="155"/>
<connect gate="G13" pin="GND" pad="165"/>
<connect gate="G14" pin="GND" pad="176"/>
<connect gate="G15" pin="GND" pad="197"/>
<connect gate="G16" pin="GND" pad="216"/>
<connect gate="G17" pin="GND" pad="232"/>
<connect gate="G18" pin="GND" pad="145"/>
<connect gate="G2" pin="GND" pad="22"/>
<connect gate="G3" pin="GND" pad="32"/>
<connect gate="G4" pin="GND" pad="42"/>
<connect gate="G5" pin="GND" pad="52"/>
<connect gate="G6" pin="GND" pad="69"/>
<connect gate="G7" pin="GND" pad="85"/>
<connect gate="G8" pin="GND" pad="93"/>
<connect gate="G9" pin="GND" pad="104"/>
<connect gate="VI1" pin="VCC" pad="5"/>
<connect gate="VI10" pin="VCC" pad="130"/>
<connect gate="VI11" pin="VCC" pad="139"/>
<connect gate="VI12" pin="VCC" pad="150"/>
<connect gate="VI13" pin="VCC" pad="159"/>
<connect gate="VI14" pin="VCC" pad="170"/>
<connect gate="VI15" pin="VCC" pad="187"/>
<connect gate="VI16" pin="VCC" pad="225"/>
<connect gate="VI2" pin="VCC" pad="20"/>
<connect gate="VI3" pin="VCC" pad="27"/>
<connect gate="VI4" pin="VCC" pad="40"/>
<connect gate="VI5" pin="VCC" pad="47"/>
<connect gate="VI6" pin="VCC" pad="76"/>
<connect gate="VI7" pin="VCC" pad="89"/>
<connect gate="VI8" pin="VCC" pad="96"/>
<connect gate="VI9" pin="VCC" pad="122"/>
<connect gate="VO1" pin="VCCIO" pad="16"/>
<connect gate="VO10" pin="VCCIO" pad="224"/>
<connect gate="VO2" pin="VCCIO" pad="37"/>
<connect gate="VO3" pin="VCCIO" pad="57"/>
<connect gate="VO4" pin="VCCIO" pad="77"/>
<connect gate="VO5" pin="VCCIO" pad="112"/>
<connect gate="VO6" pin="VCCIO" pad="140"/>
<connect gate="VO7" pin="VCCIO" pad="160"/>
<connect gate="VO8" pin="VCCIO" pad="189"/>
<connect gate="VO9" pin="VCCIO" pad="205"/>
<connect gate="_" pin="/CE" pad="178"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="121"/>
<connect gate="_" pin="/STATUS" pad="60"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="180"/>
<connect gate="_" pin="DCLK" pad="179"/>
<connect gate="_" pin="GCLK" pad="211"/>
<connect gate="_" pin="GCLK1" pad="91"/>
<connect gate="_" pin="IN0" pad="90"/>
<connect gate="_" pin="IN1" pad="92"/>
<connect gate="_" pin="IN2" pad="210"/>
<connect gate="_" pin="IN3" pad="212"/>
<connect gate="_" pin="MSEL0" pad="124"/>
<connect gate="_" pin="MSEL1" pad="123"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="177"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="58"/>
<connect gate="_" pin="TRST" pad="59"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K200SRC240-3N"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8934"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K130-BGA672" prefix="IC">
<description>&lt;b&gt;EPF10K130&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="130E672C"/>
<gate name="-A" symbol="A14-130E"/>
<gate name="-B" symbol="B14-130E"/>
<gate name="-C" symbol="C14-130E"/>
<gate name="-D" symbol="D14-130E"/>
<gate name="-E" symbol="E14-130E"/>
<gate name="-F" symbol="F13-130E"/>
<gate name="-G" symbol="G13-130E"/>
<gate name="-H" symbol="H13-130E"/>
<gate name="-I" symbol="I12-130E"/>
<gate name="-J" symbol="J13-130E"/>
<gate name="-K" symbol="K13-130E"/>
<gate name="-L" symbol="L13-130E"/>
<gate name="-M" symbol="M13-130E"/>
<gate name="-N" symbol="N13-130E"/>
<gate name="-O" symbol="O13-130E"/>
<gate name="-P" symbol="P13-130E"/>
<gate name="-1" symbol="51-130E"/>
<gate name="-2" symbol="92-130E"/>
<gate name="-3" symbol="133-130E"/>
<gate name="-4" symbol="174-130E"/>
<gate name="-5" symbol="221-130E"/>
<gate name="-6" symbol="261-130E"/>
<gate name="-7" symbol="301-130E"/>
<gate name="-8" symbol="344-130E"/>
<gate name="-9" symbol="384-130E"/>
<gate name="-10" symbol="432-130E"/>
<gate name="-11" symbol="472-130E"/>
<gate name="-12" symbol="513-130E"/>
<gate name="-13" symbol="524-130E"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="G50" symbol="GND"/>
<gate name="G51" symbol="GND"/>
<gate name="G52" symbol="GND"/>
<gate name="G53" symbol="GND"/>
<gate name="G54" symbol="GND"/>
<gate name="G55" symbol="GND"/>
<gate name="G56" symbol="GND"/>
<gate name="G57" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="V24" symbol="VCCINT"/>
<gate name="V25" symbol="VCCINT"/>
<gate name="V26" symbol="VCCINT"/>
<gate name="V27" symbol="VCCINT"/>
<gate name="V28" symbol="VCCINT"/>
<gate name="V29" symbol="VCCINT"/>
<gate name="V30" symbol="VCCIO"/>
<gate name="V31" symbol="VCCIO"/>
<gate name="V32" symbol="VCCIO"/>
<gate name="V33" symbol="VCCIO"/>
<gate name="V34" symbol="VCCIO"/>
<gate name="V35" symbol="VCCIO"/>
<gate name="V36" symbol="VCCIO"/>
<gate name="V37" symbol="VCCIO"/>
<gate name="V38" symbol="VCCIO"/>
<gate name="V39" symbol="VCCIO"/>
<gate name="V40" symbol="VCCIO"/>
<gate name="V41" symbol="VCCIO"/>
<gate name="V42" symbol="VCCIO"/>
<gate name="V43" symbol="VCCIO"/>
<gate name="V44" symbol="VCCIO"/>
<gate name="V45" symbol="VCCIO"/>
<gate name="V46" symbol="VCCIO"/>
<gate name="V47" symbol="VCCIO"/>
<gate name="V48" symbol="VCCIO"/>
<gate name="V49" symbol="VCCIO"/>
<gate name="V50" symbol="VCCIO"/>
<gate name="V51" symbol="VCCIO"/>
<gate name="V52" symbol="VCCIO"/>
<gate name="V53" symbol="VCCIO"/>
<gate name="V54" symbol="VCCIO"/>
<gate name="V55" symbol="VCCIO"/>
<gate name="V56" symbol="VCCIO"/>
<gate name="V57" symbol="VCCIO"/>
<gate name="V58" symbol="VCCIO"/>
<gate name="V59" symbol="VCCIO"/>
<gate name="V60" symbol="VCCIO"/>
<gate name="1" symbol="NC"/>
<gate name="2" symbol="NC"/>
<gate name="3" symbol="NC"/>
<gate name="4" symbol="NC"/>
<gate name="5" symbol="NC"/>
<gate name="6" symbol="NC"/>
<gate name="7" symbol="NC"/>
<gate name="8" symbol="NC"/>
<gate name="9" symbol="NC"/>
<gate name="10" symbol="NC"/>
<gate name="11" symbol="NC"/>
<gate name="12" symbol="NC"/>
<gate name="13" symbol="NC"/>
<gate name="14" symbol="NC"/>
<gate name="15" symbol="NC"/>
<gate name="16" symbol="NC"/>
<gate name="17" symbol="NC"/>
<gate name="18" symbol="NC"/>
<gate name="19" symbol="NC"/>
<gate name="20" symbol="NC"/>
<gate name="21" symbol="NC"/>
<gate name="22" symbol="NC"/>
<gate name="23" symbol="NC"/>
<gate name="24" symbol="NC"/>
<gate name="25" symbol="NC"/>
<gate name="26" symbol="NC"/>
<gate name="27" symbol="NC"/>
<gate name="28" symbol="NC"/>
<gate name="29" symbol="NC"/>
<gate name="30" symbol="NC"/>
<gate name="31" symbol="NC"/>
<gate name="32" symbol="NC"/>
<gate name="33" symbol="NC"/>
<gate name="34" symbol="NC"/>
<gate name="35" symbol="NC"/>
<gate name="36" symbol="NC"/>
<gate name="37" symbol="NC"/>
<gate name="38" symbol="NC"/>
<gate name="39" symbol="NC"/>
<gate name="40" symbol="NC"/>
<gate name="41" symbol="NC"/>
<gate name="42" symbol="NC"/>
<gate name="43" symbol="NC"/>
<gate name="44" symbol="NC"/>
<gate name="45" symbol="NC"/>
<gate name="46" symbol="NC"/>
<gate name="47" symbol="NC"/>
<gate name="48" symbol="NC"/>
<gate name="49" symbol="NC"/>
<gate name="50" symbol="NC"/>
<gate name="51" symbol="NC"/>
<gate name="52" symbol="NC"/>
<gate name="53" symbol="NC"/>
<gate name="54" symbol="NC"/>
<gate name="55" symbol="NC"/>
<gate name="56" symbol="NC"/>
<gate name="57" symbol="NC"/>
<gate name="58" symbol="NC"/>
<gate name="59" symbol="NC"/>
<gate name="60" symbol="NC"/>
<gate name="61" symbol="NC"/>
<gate name="62" symbol="NC"/>
<gate name="63" symbol="NC"/>
<gate name="64" symbol="NC"/>
<gate name="65" symbol="NC"/>
<gate name="66" symbol="NC"/>
<gate name="67" symbol="NC"/>
<gate name="68" symbol="NC"/>
<gate name="69" symbol="NC"/>
<gate name="70" symbol="NC"/>
<gate name="71" symbol="NC"/>
<gate name="72" symbol="NC"/>
<gate name="73" symbol="NC"/>
<gate name="74" symbol="NC"/>
<gate name="75" symbol="NC"/>
<gate name="76" symbol="NC"/>
<gate name="77" symbol="NC"/>
<gate name="78" symbol="NC"/>
<gate name="79" symbol="NC"/>
<gate name="80" symbol="NC"/>
<gate name="81" symbol="NC"/>
<gate name="82" symbol="NC"/>
<gate name="83" symbol="NC"/>
<gate name="84" symbol="NC"/>
<gate name="85" symbol="NC"/>
<gate name="86" symbol="NC"/>
<gate name="87" symbol="NC"/>
<gate name="88" symbol="NC"/>
<gate name="89" symbol="NC"/>
<gate name="90" symbol="NC"/>
<gate name="91" symbol="NC"/>
<gate name="92" symbol="NC"/>
<gate name="93" symbol="NC"/>
<gate name="94" symbol="NC"/>
<gate name="95" symbol="NC"/>
<gate name="96" symbol="NC"/>
<gate name="97" symbol="NC"/>
<gate name="98" symbol="NC"/>
<gate name="99" symbol="NC"/>
<gate name="100" symbol="NC"/>
<gate name="101" symbol="NC"/>
<gate name="102" symbol="NC"/>
<gate name="103" symbol="NC"/>
<gate name="104" symbol="NC"/>
<gate name="105" symbol="NC"/>
<gate name="106" symbol="NC"/>
<gate name="107" symbol="NC"/>
<gate name="108" symbol="NC"/>
<gate name="109" symbol="NC"/>
<gate name="110" symbol="NC"/>
<gate name="111" symbol="NC"/>
<gate name="112" symbol="NC"/>
<gate name="113" symbol="NC"/>
<gate name="114" symbol="NC"/>
<gate name="115" symbol="NC"/>
<gate name="116" symbol="NC"/>
<gate name="117" symbol="NC"/>
<gate name="118" symbol="NC"/>
<gate name="119" symbol="NC"/>
<gate name="120" symbol="NC"/>
<gate name="121" symbol="NC"/>
<gate name="122" symbol="NC"/>
<gate name="123" symbol="NC"/>
<gate name="124" symbol="NC"/>
<gate name="125" symbol="NC"/>
<gate name="126" symbol="NC"/>
<gate name="127" symbol="NC"/>
<gate name="128" symbol="NC"/>
</gates>
<devices>
<device name="" package="BGA672">
<connects>
<connect gate="-1" pin="IO11" pad="AD3"/>
<connect gate="-1" pin="IO12" pad="D5"/>
<connect gate="-1" pin="IO13" pad="E6"/>
<connect gate="-1" pin="IO14" pad="AB6"/>
<connect gate="-1" pin="IO21" pad="AC5"/>
<connect gate="-1" pin="IO22" pad="AC4"/>
<connect gate="-1" pin="IO23" pad="C5"/>
<connect gate="-1" pin="IO24" pad="D6"/>
<connect gate="-1" pin="IO31" pad="AD4"/>
<connect gate="-1" pin="IO32" pad="AC6"/>
<connect gate="-1" pin="IO33" pad="H9"/>
<connect gate="-1" pin="IO34" pad="J10"/>
<connect gate="-1" pin="IO41" pad="AD5"/>
<connect gate="-1" pin="IO42" pad="C6"/>
<connect gate="-1" pin="IO43" pad="AA7"/>
<connect gate="-1" pin="IO51" pad="AD6"/>
<connect gate="-10" pin="IO391" pad="C18"/>
<connect gate="-10" pin="IO392" pad="AA17"/>
<connect gate="-10" pin="IO393" pad="B18"/>
<connect gate="-10" pin="IO394" pad="AF19"/>
<connect gate="-10" pin="IO401" pad="Y17"/>
<connect gate="-10" pin="IO402" pad="AC18"/>
<connect gate="-10" pin="IO403" pad="D18"/>
<connect gate="-10" pin="IO411" pad="J16"/>
<connect gate="-10" pin="IO412" pad="AD19"/>
<connect gate="-10" pin="IO413" pad="F17"/>
<connect gate="-10" pin="IO414" pad="AB18"/>
<connect gate="-10" pin="IO421" pad="V16"/>
<connect gate="-10" pin="IO422" pad="C19"/>
<connect gate="-10" pin="IO423" pad="F18"/>
<connect gate="-10" pin="IO431" pad="AC19"/>
<connect gate="-10" pin="IO432" pad="G17"/>
<connect gate="-11" pin="IO433" pad="E18"/>
<connect gate="-11" pin="IO434" pad="AA18"/>
<connect gate="-11" pin="IO441" pad="G18"/>
<connect gate="-11" pin="IO442" pad="AD20"/>
<connect gate="-11" pin="IO443" pad="H17"/>
<connect gate="-11" pin="IO444" pad="Y18"/>
<connect gate="-11" pin="IO451" pad="W18"/>
<connect gate="-11" pin="IO452" pad="H18"/>
<connect gate="-11" pin="IO453" pad="E19"/>
<connect gate="-11" pin="IO454" pad="AB19"/>
<connect gate="-11" pin="IO461" pad="AC20"/>
<connect gate="-11" pin="IO462" pad="D20"/>
<connect gate="-11" pin="IO463" pad="C20"/>
<connect gate="-11" pin="IO464" pad="AF22"/>
<connect gate="-11" pin="IO471" pad="C21"/>
<connect gate="-11" pin="IO472" pad="AD21"/>
<connect gate="-12" pin="IO473" pad="F19"/>
<connect gate="-12" pin="IO474" pad="W19"/>
<connect gate="-12" pin="IO481" pad="AB20"/>
<connect gate="-12" pin="IO482" pad="E20"/>
<connect gate="-12" pin="IO483" pad="AA19"/>
<connect gate="-12" pin="IO491" pad="AC21"/>
<connect gate="-12" pin="IO492" pad="H19"/>
<connect gate="-12" pin="IO493" pad="D21"/>
<connect gate="-12" pin="IO494" pad="Y19"/>
<connect gate="-12" pin="IO501" pad="E21"/>
<connect gate="-12" pin="IO502" pad="G19"/>
<connect gate="-12" pin="IO503" pad="AD22"/>
<connect gate="-12" pin="IO504" pad="AA20"/>
<connect gate="-12" pin="IO511" pad="AC22"/>
<connect gate="-12" pin="IO512" pad="F20"/>
<connect gate="-12" pin="IO513" pad="C22"/>
<connect gate="-13" pin="IO514" pad="AB21"/>
<connect gate="-13" pin="IO521" pad="AB22"/>
<connect gate="-13" pin="IO522" pad="F21"/>
<connect gate="-13" pin="IO523" pad="AD23"/>
<connect gate="-13" pin="IO524" pad="D22"/>
<connect gate="-2" pin="IO52" pad="E7"/>
<connect gate="-2" pin="IO53" pad="J11"/>
<connect gate="-2" pin="IO61" pad="AC7"/>
<connect gate="-2" pin="IO62" pad="F8"/>
<connect gate="-2" pin="IO63" pad="AB7"/>
<connect gate="-2" pin="IO64" pad="A7"/>
<connect gate="-2" pin="IO71" pad="AA8"/>
<connect gate="-2" pin="IO72" pad="D8"/>
<connect gate="-2" pin="IO73" pad="E8"/>
<connect gate="-2" pin="IO74" pad="Y8"/>
<connect gate="-2" pin="IO81" pad="AB8"/>
<connect gate="-2" pin="IO82" pad="AD7"/>
<connect gate="-2" pin="IO83" pad="C7"/>
<connect gate="-2" pin="IO84" pad="H10"/>
<connect gate="-2" pin="IO91" pad="Y9"/>
<connect gate="-2" pin="IO92" pad="G8"/>
<connect gate="-3" pin="IO101" pad="AA9"/>
<connect gate="-3" pin="IO102" pad="F7"/>
<connect gate="-3" pin="IO103" pad="C9"/>
<connect gate="-3" pin="IO104" pad="AB9"/>
<connect gate="-3" pin="IO111" pad="V10"/>
<connect gate="-3" pin="IO112" pad="H8"/>
<connect gate="-3" pin="IO113" pad="W10"/>
<connect gate="-3" pin="IO121" pad="AD8"/>
<connect gate="-3" pin="IO122" pad="D9"/>
<connect gate="-3" pin="IO123" pad="G9"/>
<connect gate="-3" pin="IO124" pad="Y10"/>
<connect gate="-3" pin="IO131" pad="AA10"/>
<connect gate="-3" pin="IO132" pad="F9"/>
<connect gate="-3" pin="IO133" pad="E10"/>
<connect gate="-3" pin="IO93" pad="E9"/>
<connect gate="-3" pin="IO94" pad="W9"/>
<connect gate="-4" pin="IO141" pad="AD9"/>
<connect gate="-4" pin="IO142" pad="F10"/>
<connect gate="-4" pin="IO143" pad="J9"/>
<connect gate="-4" pin="IO144" pad="AC9"/>
<connect gate="-4" pin="IO151" pad="U12"/>
<connect gate="-4" pin="IO152" pad="G10"/>
<connect gate="-4" pin="IO153" pad="D10"/>
<connect gate="-4" pin="IO154" pad="V11"/>
<connect gate="-4" pin="IO161" pad="AA11"/>
<connect gate="-4" pin="IO162" pad="H11"/>
<connect gate="-4" pin="IO163" pad="G11"/>
<connect gate="-4" pin="IO164" pad="AC10"/>
<connect gate="-4" pin="IO171" pad="F11"/>
<connect gate="-4" pin="IO172" pad="AD10"/>
<connect gate="-4" pin="IO173" pad="E11"/>
<connect gate="-4" pin="IO174" pad="Y11"/>
<connect gate="-5" pin="IO181" pad="W11"/>
<connect gate="-5" pin="IO182" pad="C11"/>
<connect gate="-5" pin="IO183" pad="K12"/>
<connect gate="-5" pin="IO184" pad="AB11"/>
<connect gate="-5" pin="IO191" pad="AC11"/>
<connect gate="-5" pin="IO192" pad="D11"/>
<connect gate="-5" pin="IO193" pad="H12"/>
<connect gate="-5" pin="IO201" pad="AD11"/>
<connect gate="-5" pin="IO202" pad="K14"/>
<connect gate="-5" pin="IO203" pad="J12"/>
<connect gate="-5" pin="IO204" pad="V12"/>
<connect gate="-5" pin="IO211" pad="Y12"/>
<connect gate="-5" pin="IO212" pad="C12"/>
<connect gate="-5" pin="IO213" pad="F12"/>
<connect gate="-5" pin="IO214" pad="W12"/>
<connect gate="-5" pin="IO221" pad="E12"/>
<connect gate="-6" pin="IO222" pad="D12"/>
<connect gate="-6" pin="IO223" pad="AA12"/>
<connect gate="-6" pin="IO224" pad="AB12"/>
<connect gate="-6" pin="IO231" pad="AD12"/>
<connect gate="-6" pin="IO232" pad="G12"/>
<connect gate="-6" pin="IO233" pad="H13"/>
<connect gate="-6" pin="IO234" pad="AC12"/>
<connect gate="-6" pin="IO241" pad="V13"/>
<connect gate="-6" pin="IO242" pad="G13"/>
<connect gate="-6" pin="IO243" pad="J14"/>
<connect gate="-6" pin="IO244" pad="U13"/>
<connect gate="-6" pin="IO251" pad="AB13"/>
<connect gate="-6" pin="IO252" pad="C13"/>
<connect gate="-6" pin="IO253" pad="F13"/>
<connect gate="-6" pin="IO254" pad="W13"/>
<connect gate="-6" pin="IO261" pad="AE13"/>
<connect gate="-7" pin="IO262" pad="D13"/>
<connect gate="-7" pin="IO263" pad="J13"/>
<connect gate="-7" pin="IO264" pad="AC13"/>
<connect gate="-7" pin="IO271" pad="AA14"/>
<connect gate="-7" pin="IO272" pad="AD14"/>
<connect gate="-7" pin="IO273" pad="H14"/>
<connect gate="-7" pin="IO274" pad="C14"/>
<connect gate="-7" pin="IO281" pad="Y14"/>
<connect gate="-7" pin="IO282" pad="D14"/>
<connect gate="-7" pin="IO283" pad="E14"/>
<connect gate="-7" pin="IO284" pad="AB14"/>
<connect gate="-7" pin="IO291" pad="AC15"/>
<connect gate="-7" pin="IO292" pad="W14"/>
<connect gate="-7" pin="IO293" pad="D15"/>
<connect gate="-7" pin="IO294" pad="B15"/>
<connect gate="-7" pin="IO301" pad="U15"/>
<connect gate="-8" pin="IO302" pad="F15"/>
<connect gate="-8" pin="IO303" pad="V14"/>
<connect gate="-8" pin="IO311" pad="Y15"/>
<connect gate="-8" pin="IO312" pad="E15"/>
<connect gate="-8" pin="IO313" pad="G15"/>
<connect gate="-8" pin="IO314" pad="AB15"/>
<connect gate="-8" pin="IO321" pad="AD16"/>
<connect gate="-8" pin="IO322" pad="C16"/>
<connect gate="-8" pin="IO323" pad="AA15"/>
<connect gate="-8" pin="IO331" pad="V15"/>
<connect gate="-8" pin="IO332" pad="W15"/>
<connect gate="-8" pin="IO333" pad="D16"/>
<connect gate="-8" pin="IO341" pad="Y16"/>
<connect gate="-8" pin="IO342" pad="AC16"/>
<connect gate="-8" pin="IO343" pad="H15"/>
<connect gate="-8" pin="IO344" pad="B17"/>
<connect gate="-9" pin="IO351" pad="AA16"/>
<connect gate="-9" pin="IO352" pad="E16"/>
<connect gate="-9" pin="IO353" pad="J15"/>
<connect gate="-9" pin="IO354" pad="AB16"/>
<connect gate="-9" pin="IO361" pad="W17"/>
<connect gate="-9" pin="IO362" pad="C17"/>
<connect gate="-9" pin="IO363" pad="K15"/>
<connect gate="-9" pin="IO364" pad="AD17"/>
<connect gate="-9" pin="IO371" pad="D17"/>
<connect gate="-9" pin="IO372" pad="AC17"/>
<connect gate="-9" pin="IO373" pad="F16"/>
<connect gate="-9" pin="IO374" pad="W16"/>
<connect gate="-9" pin="IO381" pad="AB17"/>
<connect gate="-9" pin="IO382" pad="H16"/>
<connect gate="-9" pin="IO383" pad="G16"/>
<connect gate="-9" pin="IO384" pad="AE18"/>
<connect gate="-A" pin="IOA1" pad="C23"/>
<connect gate="-A" pin="IOA10" pad="F5"/>
<connect gate="-A" pin="IOA11" pad="G5"/>
<connect gate="-A" pin="IOA12" pad="G22"/>
<connect gate="-A" pin="IOA13" pad="C2"/>
<connect gate="-A" pin="IOA14" pad="B1"/>
<connect gate="-A" pin="IOA2" pad="E24"/>
<connect gate="-A" pin="IOA3" pad="F22"/>
<connect gate="-A" pin="IOA4" pad="E22"/>
<connect gate="-A" pin="IOA5" pad="J20"/>
<connect gate="-A" pin="IOA6" pad="F4"/>
<connect gate="-A" pin="IOA7" pad="C4"/>
<connect gate="-A" pin="IOA8" pad="E3"/>
<connect gate="-A" pin="IOA9" pad="E5"/>
<connect gate="-B" pin="IOB1" pad="F23"/>
<connect gate="-B" pin="IOB10" pad="H22"/>
<connect gate="-B" pin="IOB11" pad="J19"/>
<connect gate="-B" pin="IOB12" pad="K18"/>
<connect gate="-B" pin="IOB13" pad="F2"/>
<connect gate="-B" pin="IOB14" pad="E2"/>
<connect gate="-B" pin="IOB2" pad="F24"/>
<connect gate="-B" pin="IOB3" pad="J18"/>
<connect gate="-B" pin="IOB4" pad="G24"/>
<connect gate="-B" pin="IOB5" pad="H6"/>
<connect gate="-B" pin="IOB6" pad="G4"/>
<connect gate="-B" pin="IOB7" pad="F3"/>
<connect gate="-B" pin="IOB8" pad="H4"/>
<connect gate="-B" pin="IOB9" pad="H5"/>
<connect gate="-C" pin="IOC1" pad="H23"/>
<connect gate="-C" pin="IOC10" pad="J22"/>
<connect gate="-C" pin="IOC11" pad="K20"/>
<connect gate="-C" pin="IOC12" pad="K21"/>
<connect gate="-C" pin="IOC13" pad="F26"/>
<connect gate="-C" pin="IOC14" pad="G2"/>
<connect gate="-C" pin="IOC2" pad="J21"/>
<connect gate="-C" pin="IOC3" pad="K19"/>
<connect gate="-C" pin="IOC4" pad="J8"/>
<connect gate="-C" pin="IOC5" pad="J7"/>
<connect gate="-C" pin="IOC6" pad="H3"/>
<connect gate="-C" pin="IOC7" pad="H24"/>
<connect gate="-C" pin="IOC8" pad="J4"/>
<connect gate="-C" pin="IOC9" pad="J6"/>
<connect gate="-D" pin="IOD1" pad="H26"/>
<connect gate="-D" pin="IOD10" pad="K8"/>
<connect gate="-D" pin="IOD11" pad="L18"/>
<connect gate="-D" pin="IOD12" pad="L20"/>
<connect gate="-D" pin="IOD13" pad="G1"/>
<connect gate="-D" pin="IOD14" pad="J2"/>
<connect gate="-D" pin="IOD3" pad="J24"/>
<connect gate="-D" pin="IOD4" pad="L19"/>
<connect gate="-D" pin="IOD6" pad="K5"/>
<connect gate="-D" pin="IOD7" pad="K3"/>
<connect gate="-D" pin="IOD8" pad="K6"/>
<connect gate="-D" pin="IOD9" pad="K7"/>
<connect gate="-E" pin="IOE1" pad="L21"/>
<connect gate="-E" pin="IOE10" pad="M17"/>
<connect gate="-E" pin="IOE11" pad="M18"/>
<connect gate="-E" pin="IOE12" pad="K25"/>
<connect gate="-E" pin="IOE13" pad="K2"/>
<connect gate="-E" pin="IOE14" pad="K1"/>
<connect gate="-E" pin="IOE2" pad="L4"/>
<connect gate="-E" pin="IOE3" pad="L5"/>
<connect gate="-E" pin="IOE4" pad="L6"/>
<connect gate="-E" pin="IOE5" pad="L9"/>
<connect gate="-E" pin="IOE6" pad="L7"/>
<connect gate="-E" pin="IOE7" pad="K9"/>
<connect gate="-E" pin="IOE8" pad="K23"/>
<connect gate="-E" pin="IOE9" pad="K24"/>
<connect gate="-F" pin="IOF1" pad="L23"/>
<connect gate="-F" pin="IOF10" pad="M19"/>
<connect gate="-F" pin="IOF11" pad="M20"/>
<connect gate="-F" pin="IOF12" pad="M21"/>
<connect gate="-F" pin="IOF13" pad="L1"/>
<connect gate="-F" pin="IOF2" pad="N17"/>
<connect gate="-F" pin="IOF3" pad="M4"/>
<connect gate="-F" pin="IOF4" pad="M7"/>
<connect gate="-F" pin="IOF5" pad="L8"/>
<connect gate="-F" pin="IOF6" pad="L3"/>
<connect gate="-F" pin="IOF7" pad="L24"/>
<connect gate="-F" pin="IOF8" pad="M3"/>
<connect gate="-F" pin="IOF9" pad="M6"/>
<connect gate="-G" pin="IOG1" pad="N19"/>
<connect gate="-G" pin="IOG10" pad="N20"/>
<connect gate="-G" pin="IOG11" pad="L26"/>
<connect gate="-G" pin="IOG12" pad="M26"/>
<connect gate="-G" pin="IOG13" pad="M1"/>
<connect gate="-G" pin="IOG2" pad="M23"/>
<connect gate="-G" pin="IOG3" pad="M24"/>
<connect gate="-G" pin="IOG4" pad="N7"/>
<connect gate="-G" pin="IOG5" pad="M9"/>
<connect gate="-G" pin="IOG6" pad="M8"/>
<connect gate="-G" pin="IOG7" pad="M10"/>
<connect gate="-G" pin="IOG8" pad="N3"/>
<connect gate="-G" pin="IOG9" pad="N4"/>
<connect gate="-H" pin="IOH1" pad="N24"/>
<connect gate="-H" pin="IOH10" pad="P5"/>
<connect gate="-H" pin="IOH11" pad="N26"/>
<connect gate="-H" pin="IOH12" pad="N1"/>
<connect gate="-H" pin="IOH13" pad="N25"/>
<connect gate="-H" pin="IOH2" pad="N22"/>
<connect gate="-H" pin="IOH3" pad="N21"/>
<connect gate="-H" pin="IOH4" pad="P4"/>
<connect gate="-H" pin="IOH5" pad="N6"/>
<connect gate="-H" pin="IOH6" pad="N5"/>
<connect gate="-H" pin="IOH7" pad="N9"/>
<connect gate="-H" pin="IOH8" pad="N23"/>
<connect gate="-H" pin="IOH9" pad="P3"/>
<connect gate="-I" pin="IOI1" pad="P24"/>
<connect gate="-I" pin="IOI10" pad="R3"/>
<connect gate="-I" pin="IOI11" pad="P26"/>
<connect gate="-I" pin="IOI12" pad="P25"/>
<connect gate="-I" pin="IOI2" pad="P23"/>
<connect gate="-I" pin="IOI3" pad="R4"/>
<connect gate="-I" pin="IOI4" pad="N8"/>
<connect gate="-I" pin="IOI5" pad="P6"/>
<connect gate="-I" pin="IOI6" pad="N18"/>
<connect gate="-I" pin="IOI7" pad="P7"/>
<connect gate="-I" pin="IOI8" pad="P8"/>
<connect gate="-I" pin="IOI9" pad="P21"/>
<connect gate="-J" pin="IOJ1" pad="P20"/>
<connect gate="-J" pin="IOJ10" pad="T4"/>
<connect gate="-J" pin="IOJ11" pad="T26"/>
<connect gate="-J" pin="IOJ12" pad="R25"/>
<connect gate="-J" pin="IOJ13" pad="R2"/>
<connect gate="-J" pin="IOJ2" pad="T24"/>
<connect gate="-J" pin="IOJ3" pad="N10"/>
<connect gate="-J" pin="IOJ4" pad="P9"/>
<connect gate="-J" pin="IOJ5" pad="P19"/>
<connect gate="-J" pin="IOJ6" pad="R6"/>
<connect gate="-J" pin="IOJ7" pad="R23"/>
<connect gate="-J" pin="IOJ8" pad="R24"/>
<connect gate="-J" pin="IOJ9" pad="T3"/>
<connect gate="-K" pin="IOK1" pad="P18"/>
<connect gate="-K" pin="IOK10" pad="T23"/>
<connect gate="-K" pin="IOK11" pad="U4"/>
<connect gate="-K" pin="IOK12" pad="U26"/>
<connect gate="-K" pin="IOK13" pad="U2"/>
<connect gate="-K" pin="IOK2" pad="T22"/>
<connect gate="-K" pin="IOK3" pad="T5"/>
<connect gate="-K" pin="IOK4" pad="R7"/>
<connect gate="-K" pin="IOK5" pad="P10"/>
<connect gate="-K" pin="IOK6" pad="P17"/>
<connect gate="-K" pin="IOK7" pad="R8"/>
<connect gate="-K" pin="IOK8" pad="R21"/>
<connect gate="-K" pin="IOK9" pad="T6"/>
<connect gate="-L" pin="IOL1" pad="U22"/>
<connect gate="-L" pin="IOL10" pad="U23"/>
<connect gate="-L" pin="IOL11" pad="V2"/>
<connect gate="-L" pin="IOL12" pad="W26"/>
<connect gate="-L" pin="IOL13" pad="V25"/>
<connect gate="-L" pin="IOL2" pad="U5"/>
<connect gate="-L" pin="IOL3" pad="T7"/>
<connect gate="-L" pin="IOL4" pad="R9"/>
<connect gate="-L" pin="IOL5" pad="R10"/>
<connect gate="-L" pin="IOL6" pad="R17"/>
<connect gate="-L" pin="IOL7" pad="R20"/>
<connect gate="-L" pin="IOL8" pad="T21"/>
<connect gate="-L" pin="IOL9" pad="U6"/>
<connect gate="-M" pin="IOM1" pad="R19"/>
<connect gate="-M" pin="IOM10" pad="V23"/>
<connect gate="-M" pin="IOM11" pad="W3"/>
<connect gate="-M" pin="IOM12" pad="W24"/>
<connect gate="-M" pin="IOM13" pad="W25"/>
<connect gate="-M" pin="IOM2" pad="R18"/>
<connect gate="-M" pin="IOM3" pad="T8"/>
<connect gate="-M" pin="IOM4" pad="W2"/>
<connect gate="-M" pin="IOM5" pad="T18"/>
<connect gate="-M" pin="IOM6" pad="U7"/>
<connect gate="-M" pin="IOM7" pad="U21"/>
<connect gate="-M" pin="IOM8" pad="V4"/>
<connect gate="-M" pin="IOM9" pad="V6"/>
<connect gate="-N" pin="ION1" pad="T20"/>
<connect gate="-N" pin="ION10" pad="V22"/>
<connect gate="-N" pin="ION11" pad="Y3"/>
<connect gate="-N" pin="ION12" pad="Y25"/>
<connect gate="-N" pin="ION13" pad="Y1"/>
<connect gate="-N" pin="ION2" pad="W23"/>
<connect gate="-N" pin="ION3" pad="T9"/>
<connect gate="-N" pin="ION4" pad="W4"/>
<connect gate="-N" pin="ION5" pad="T19"/>
<connect gate="-N" pin="ION6" pad="U8"/>
<connect gate="-N" pin="ION7" pad="U9"/>
<connect gate="-N" pin="ION8" pad="U20"/>
<connect gate="-N" pin="ION9" pad="V21"/>
<connect gate="-O" pin="IOO1" pad="W21"/>
<connect gate="-O" pin="IOO10" pad="Y4"/>
<connect gate="-O" pin="IOO11" pad="Y23"/>
<connect gate="-O" pin="IOO12" pad="AA24"/>
<connect gate="-O" pin="IOO13" pad="AB1"/>
<connect gate="-O" pin="IOO2" pad="Y22"/>
<connect gate="-O" pin="IOO3" pad="V8"/>
<connect gate="-O" pin="IOO4" pad="V7"/>
<connect gate="-O" pin="IOO5" pad="U19"/>
<connect gate="-O" pin="IOO6" pad="V20"/>
<connect gate="-O" pin="IOO7" pad="W5"/>
<connect gate="-O" pin="IOO8" pad="W7"/>
<connect gate="-O" pin="IOO9" pad="W22"/>
<connect gate="-P" pin="IOP1" pad="AD25"/>
<connect gate="-P" pin="IOP10" pad="V19"/>
<connect gate="-P" pin="IOP11" pad="W8"/>
<connect gate="-P" pin="IOP12" pad="AA3"/>
<connect gate="-P" pin="IOP13" pad="AD1"/>
<connect gate="-P" pin="IOP2" pad="Y20"/>
<connect gate="-P" pin="IOP3" pad="AA5"/>
<connect gate="-P" pin="IOP4" pad="AA6"/>
<connect gate="-P" pin="IOP5" pad="AA4"/>
<connect gate="-P" pin="IOP6" pad="AC23"/>
<connect gate="-P" pin="IOP7" pad="AD24"/>
<connect gate="-P" pin="IOP8" pad="U18"/>
<connect gate="-P" pin="IOP9" pad="V18"/>
<connect gate="1" pin="NC" pad="AA1"/>
<connect gate="10" pin="NC" pad="AC26"/>
<connect gate="100" pin="NC" pad="D2"/>
<connect gate="101" pin="NC" pad="D25"/>
<connect gate="102" pin="NC" pad="D26"/>
<connect gate="103" pin="NC" pad="E1"/>
<connect gate="104" pin="NC" pad="E25"/>
<connect gate="105" pin="NC" pad="E26"/>
<connect gate="106" pin="NC" pad="F1"/>
<connect gate="107" pin="NC" pad="F25"/>
<connect gate="108" pin="NC" pad="G25"/>
<connect gate="109" pin="NC" pad="G26"/>
<connect gate="11" pin="NC" pad="AD2"/>
<connect gate="110" pin="NC" pad="H1"/>
<connect gate="111" pin="NC" pad="J1"/>
<connect gate="112" pin="NC" pad="J25"/>
<connect gate="113" pin="NC" pad="J26"/>
<connect gate="114" pin="NC" pad="K26"/>
<connect gate="115" pin="NC" pad="L2"/>
<connect gate="116" pin="NC" pad="L25"/>
<connect gate="117" pin="NC" pad="N2"/>
<connect gate="118" pin="NC" pad="P1"/>
<connect gate="119" pin="NC" pad="P2"/>
<connect gate="12" pin="NC" pad="AD26"/>
<connect gate="120" pin="NC" pad="R1"/>
<connect gate="121" pin="NC" pad="R26"/>
<connect gate="122" pin="NC" pad="T1"/>
<connect gate="123" pin="NC" pad="U1"/>
<connect gate="124" pin="NC" pad="U25"/>
<connect gate="125" pin="NC" pad="V1"/>
<connect gate="126" pin="NC" pad="V26"/>
<connect gate="127" pin="NC" pad="W1"/>
<connect gate="128" pin="NC" pad="Y26"/>
<connect gate="13" pin="NC" pad="AE1"/>
<connect gate="14" pin="NC" pad="AE3"/>
<connect gate="15" pin="NC" pad="AE4"/>
<connect gate="16" pin="NC" pad="AE5"/>
<connect gate="17" pin="NC" pad="AE6"/>
<connect gate="18" pin="NC" pad="AE7"/>
<connect gate="19" pin="NC" pad="AE8"/>
<connect gate="2" pin="NC" pad="AA2"/>
<connect gate="20" pin="NC" pad="AE9"/>
<connect gate="21" pin="NC" pad="AE10"/>
<connect gate="22" pin="NC" pad="AE11"/>
<connect gate="23" pin="NC" pad="AE12"/>
<connect gate="24" pin="NC" pad="AE14"/>
<connect gate="25" pin="NC" pad="AE15"/>
<connect gate="26" pin="NC" pad="AE16"/>
<connect gate="27" pin="NC" pad="AE17"/>
<connect gate="28" pin="NC" pad="AE19"/>
<connect gate="29" pin="NC" pad="AE20"/>
<connect gate="3" pin="NC" pad="AA25"/>
<connect gate="30" pin="NC" pad="AE21"/>
<connect gate="31" pin="NC" pad="AE22"/>
<connect gate="32" pin="NC" pad="AE23"/>
<connect gate="33" pin="NC" pad="AE24"/>
<connect gate="34" pin="NC" pad="AE26"/>
<connect gate="35" pin="NC" pad="AF3"/>
<connect gate="36" pin="NC" pad="AF4"/>
<connect gate="37" pin="NC" pad="AF5"/>
<connect gate="38" pin="NC" pad="AF6"/>
<connect gate="39" pin="NC" pad="AF7"/>
<connect gate="4" pin="NC" pad="AB2"/>
<connect gate="40" pin="NC" pad="AF8"/>
<connect gate="41" pin="NC" pad="AF9"/>
<connect gate="42" pin="NC" pad="AF10"/>
<connect gate="43" pin="NC" pad="AF11"/>
<connect gate="44" pin="NC" pad="AF12"/>
<connect gate="45" pin="NC" pad="AF13"/>
<connect gate="46" pin="NC" pad="AF14"/>
<connect gate="47" pin="NC" pad="AF15"/>
<connect gate="48" pin="NC" pad="AF16"/>
<connect gate="49" pin="NC" pad="AF17"/>
<connect gate="5" pin="NC" pad="AB25"/>
<connect gate="50" pin="NC" pad="AF18"/>
<connect gate="51" pin="NC" pad="AF20"/>
<connect gate="52" pin="NC" pad="AF21"/>
<connect gate="53" pin="NC" pad="AF23"/>
<connect gate="54" pin="NC" pad="AF24"/>
<connect gate="55" pin="NC" pad="A3"/>
<connect gate="56" pin="NC" pad="A4"/>
<connect gate="57" pin="NC" pad="A5"/>
<connect gate="58" pin="NC" pad="A6"/>
<connect gate="59" pin="NC" pad="A8"/>
<connect gate="6" pin="NC" pad="AB26"/>
<connect gate="60" pin="NC" pad="A9"/>
<connect gate="61" pin="NC" pad="A10"/>
<connect gate="62" pin="NC" pad="A11"/>
<connect gate="63" pin="NC" pad="A12"/>
<connect gate="64" pin="NC" pad="A13"/>
<connect gate="65" pin="NC" pad="A14"/>
<connect gate="66" pin="NC" pad="A15"/>
<connect gate="67" pin="NC" pad="A16"/>
<connect gate="68" pin="NC" pad="A17"/>
<connect gate="69" pin="NC" pad="A18"/>
<connect gate="7" pin="NC" pad="AC1"/>
<connect gate="70" pin="NC" pad="A19"/>
<connect gate="71" pin="NC" pad="A20"/>
<connect gate="72" pin="NC" pad="A21"/>
<connect gate="73" pin="NC" pad="A22"/>
<connect gate="74" pin="NC" pad="A23"/>
<connect gate="75" pin="NC" pad="A24"/>
<connect gate="76" pin="NC" pad="B3"/>
<connect gate="77" pin="NC" pad="B4"/>
<connect gate="78" pin="NC" pad="B5"/>
<connect gate="79" pin="NC" pad="B6"/>
<connect gate="8" pin="NC" pad="AC2"/>
<connect gate="80" pin="NC" pad="B7"/>
<connect gate="81" pin="NC" pad="B8"/>
<connect gate="82" pin="NC" pad="B9"/>
<connect gate="83" pin="NC" pad="B10"/>
<connect gate="84" pin="NC" pad="B11"/>
<connect gate="85" pin="NC" pad="B12"/>
<connect gate="86" pin="NC" pad="B13"/>
<connect gate="87" pin="NC" pad="B14"/>
<connect gate="88" pin="NC" pad="B16"/>
<connect gate="89" pin="NC" pad="B19"/>
<connect gate="9" pin="NC" pad="AC25"/>
<connect gate="90" pin="NC" pad="B20"/>
<connect gate="91" pin="NC" pad="B21"/>
<connect gate="92" pin="NC" pad="B22"/>
<connect gate="93" pin="NC" pad="B23"/>
<connect gate="94" pin="NC" pad="B24"/>
<connect gate="95" pin="NC" pad="B26"/>
<connect gate="96" pin="NC" pad="C1"/>
<connect gate="97" pin="NC" pad="C25"/>
<connect gate="98" pin="NC" pad="C26"/>
<connect gate="99" pin="NC" pad="D1"/>
<connect gate="G1" pin="GND" pad="AA13"/>
<connect gate="G10" pin="GND" pad="AC24"/>
<connect gate="G11" pin="GND" pad="AD13"/>
<connect gate="G12" pin="GND" pad="AD18"/>
<connect gate="G13" pin="GND" pad="AE2"/>
<connect gate="G14" pin="GND" pad="AE25"/>
<connect gate="G15" pin="GND" pad="AF2"/>
<connect gate="G16" pin="GND" pad="AF25"/>
<connect gate="G17" pin="GND" pad="A2"/>
<connect gate="G18" pin="GND" pad="A25"/>
<connect gate="G19" pin="GND" pad="B2"/>
<connect gate="G2" pin="GND" pad="AA22"/>
<connect gate="G20" pin="GND" pad="B25"/>
<connect gate="G21" pin="GND" pad="C3"/>
<connect gate="G22" pin="GND" pad="C10"/>
<connect gate="G23" pin="GND" pad="C24"/>
<connect gate="G24" pin="GND" pad="D3"/>
<connect gate="G25" pin="GND" pad="D4"/>
<connect gate="G26" pin="GND" pad="D19"/>
<connect gate="G27" pin="GND" pad="D23"/>
<connect gate="G28" pin="GND" pad="D24"/>
<connect gate="G29" pin="GND" pad="E4"/>
<connect gate="G3" pin="GND" pad="AB3"/>
<connect gate="G30" pin="GND" pad="E23"/>
<connect gate="G31" pin="GND" pad="G23"/>
<connect gate="G32" pin="GND" pad="J5"/>
<connect gate="G33" pin="GND" pad="J23"/>
<connect gate="G34" pin="GND" pad="K4"/>
<connect gate="G35" pin="GND" pad="K10"/>
<connect gate="G36" pin="GND" pad="K17"/>
<connect gate="G37" pin="GND" pad="L11"/>
<connect gate="G38" pin="GND" pad="L16"/>
<connect gate="G39" pin="GND" pad="L22"/>
<connect gate="G4" pin="GND" pad="AB4"/>
<connect gate="G40" pin="GND" pad="M5"/>
<connect gate="G41" pin="GND" pad="M12"/>
<connect gate="G42" pin="GND" pad="M14"/>
<connect gate="G43" pin="GND" pad="M15"/>
<connect gate="G44" pin="GND" pad="N13"/>
<connect gate="G45" pin="GND" pad="N14"/>
<connect gate="G46" pin="GND" pad="P13"/>
<connect gate="G47" pin="GND" pad="P14"/>
<connect gate="G48" pin="GND" pad="P22"/>
<connect gate="G49" pin="GND" pad="R12"/>
<connect gate="G5" pin="GND" pad="AB5"/>
<connect gate="G50" pin="GND" pad="R15"/>
<connect gate="G51" pin="GND" pad="T11"/>
<connect gate="G52" pin="GND" pad="T16"/>
<connect gate="G53" pin="GND" pad="U10"/>
<connect gate="G54" pin="GND" pad="U17"/>
<connect gate="G55" pin="GND" pad="U24"/>
<connect gate="G56" pin="GND" pad="V3"/>
<connect gate="G57" pin="GND" pad="Y5"/>
<connect gate="G6" pin="GND" pad="AB23"/>
<connect gate="G7" pin="GND" pad="AB24"/>
<connect gate="G8" pin="GND" pad="AC3"/>
<connect gate="G9" pin="GND" pad="AC8"/>
<connect gate="V1" pin="VCC" pad="AA23"/>
<connect gate="V10" pin="VCC" pad="L12"/>
<connect gate="V11" pin="VCC" pad="L14"/>
<connect gate="V12" pin="VCC" pad="L17"/>
<connect gate="V13" pin="VCC" pad="M2"/>
<connect gate="V14" pin="VCC" pad="M25"/>
<connect gate="V15" pin="VCC" pad="N11"/>
<connect gate="V16" pin="VCC" pad="N12"/>
<connect gate="V17" pin="VCC" pad="N15"/>
<connect gate="V18" pin="VCC" pad="P12"/>
<connect gate="V19" pin="VCC" pad="P15"/>
<connect gate="V2" pin="VCC" pad="AB10"/>
<connect gate="V20" pin="VCC" pad="P16"/>
<connect gate="V21" pin="VCC" pad="R14"/>
<connect gate="V22" pin="VCC" pad="T2"/>
<connect gate="V23" pin="VCC" pad="T10"/>
<connect gate="V24" pin="VCC" pad="T12"/>
<connect gate="V25" pin="VCC" pad="T14"/>
<connect gate="V26" pin="VCC" pad="T17"/>
<connect gate="V27" pin="VCC" pad="T25"/>
<connect gate="V28" pin="VCC" pad="U16"/>
<connect gate="V29" pin="VCC" pad="Y7"/>
<connect gate="V3" pin="VCC" pad="AC14"/>
<connect gate="V30" pin="VCCIO" pad="AA26"/>
<connect gate="V31" pin="VCCIO" pad="AD15"/>
<connect gate="V32" pin="VCCIO" pad="C8"/>
<connect gate="V33" pin="VCCIO" pad="C15"/>
<connect gate="V34" pin="VCCIO" pad="D7"/>
<connect gate="V35" pin="VCCIO" pad="G3"/>
<connect gate="V36" pin="VCCIO" pad="J3"/>
<connect gate="V37" pin="VCCIO" pad="J17"/>
<connect gate="V38" pin="VCCIO" pad="K11"/>
<connect gate="V39" pin="VCCIO" pad="K22"/>
<connect gate="V4" pin="VCC" pad="E13"/>
<connect gate="V40" pin="VCCIO" pad="L13"/>
<connect gate="V41" pin="VCCIO" pad="L15"/>
<connect gate="V42" pin="VCCIO" pad="M11"/>
<connect gate="V43" pin="VCCIO" pad="M13"/>
<connect gate="V44" pin="VCCIO" pad="M16"/>
<connect gate="V45" pin="VCCIO" pad="M22"/>
<connect gate="V46" pin="VCCIO" pad="N16"/>
<connect gate="V47" pin="VCCIO" pad="P11"/>
<connect gate="V48" pin="VCCIO" pad="R5"/>
<connect gate="V49" pin="VCCIO" pad="R11"/>
<connect gate="V5" pin="VCC" pad="E17"/>
<connect gate="V50" pin="VCCIO" pad="R13"/>
<connect gate="V51" pin="VCCIO" pad="R16"/>
<connect gate="V52" pin="VCCIO" pad="R22"/>
<connect gate="V53" pin="VCCIO" pad="T15"/>
<connect gate="V54" pin="VCCIO" pad="U3"/>
<connect gate="V55" pin="VCCIO" pad="U11"/>
<connect gate="V56" pin="VCCIO" pad="V5"/>
<connect gate="V57" pin="VCCIO" pad="V17"/>
<connect gate="V58" pin="VCCIO" pad="V24"/>
<connect gate="V59" pin="VCCIO" pad="Y2"/>
<connect gate="V6" pin="VCC" pad="H2"/>
<connect gate="V60" pin="VCCIO" pad="Y24"/>
<connect gate="V7" pin="VCC" pad="H25"/>
<connect gate="V8" pin="VCC" pad="K16"/>
<connect gate="V9" pin="VCC" pad="L10"/>
<connect gate="_" pin="/CE" pad="G6"/>
<connect gate="_" pin="/CEO" pad="G21"/>
<connect gate="_" pin="/CONFIG" pad="V9"/>
<connect gate="_" pin="/STATUS" pad="AA21"/>
<connect gate="_" pin="CONF_DONE" pad="H20"/>
<connect gate="_" pin="DATA0" pad="F6"/>
<connect gate="_" pin="DCLK" pad="G7"/>
<connect gate="_" pin="GCLK0" pad="T13"/>
<connect gate="_" pin="GCLK1" pad="F14"/>
<connect gate="_" pin="IN0" pad="U14"/>
<connect gate="_" pin="IN1" pad="Y13"/>
<connect gate="_" pin="IN2" pad="K13"/>
<connect gate="_" pin="IN3" pad="G14"/>
<connect gate="_" pin="MSEL0" pad="W6"/>
<connect gate="_" pin="MSEL1" pad="Y6"/>
<connect gate="_" pin="TCK" pad="G20"/>
<connect gate="_" pin="TDI" pad="H7"/>
<connect gate="_" pin="TDO" pad="H21"/>
<connect gate="_" pin="TMS" pad="W20"/>
<connect gate="_" pin="TRST" pad="Y21"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K130EFC672-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8863"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K130V-BGA600" prefix="IC">
<description>&lt;b&gt;EPF10K130&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="130V600C"/>
<gate name="-A" symbol="A16"/>
<gate name="-B" symbol="B16"/>
<gate name="-C" symbol="C16"/>
<gate name="-D" symbol="D16"/>
<gate name="-E" symbol="E16"/>
<gate name="-F" symbol="F16"/>
<gate name="-G" symbol="G16"/>
<gate name="-H" symbol="H16"/>
<gate name="-I" symbol="I16"/>
<gate name="-J" symbol="J16"/>
<gate name="-K" symbol="K16"/>
<gate name="-L" symbol="L16"/>
<gate name="-M" symbol="M16"/>
<gate name="-N" symbol="N16"/>
<gate name="-O" symbol="O16"/>
<gate name="-P" symbol="P16"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="-10" symbol="IO404"/>
<gate name="-11" symbol="IO444"/>
<gate name="-12" symbol="IO484"/>
<gate name="-13" symbol="IO524"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="G50" symbol="GND"/>
<gate name="G51" symbol="GND"/>
<gate name="G52" symbol="GND"/>
<gate name="G53" symbol="GND"/>
<gate name="G54" symbol="GND"/>
<gate name="G55" symbol="GND"/>
<gate name="G56" symbol="GND"/>
<gate name="G57" symbol="GND"/>
<gate name="G58" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="V24" symbol="VCCINT"/>
<gate name="V25" symbol="VCCINT"/>
<gate name="V26" symbol="VCCINT"/>
<gate name="V27" symbol="VCCINT"/>
<gate name="V28" symbol="VCCINT"/>
<gate name="V29" symbol="VCCINT"/>
<gate name="V30" symbol="VCCIO"/>
<gate name="V31" symbol="VCCIO"/>
<gate name="V32" symbol="VCCIO"/>
<gate name="V33" symbol="VCCIO"/>
<gate name="V34" symbol="VCCIO"/>
<gate name="V35" symbol="VCCIO"/>
<gate name="V36" symbol="VCCIO"/>
<gate name="V37" symbol="VCCIO"/>
<gate name="V38" symbol="VCCIO"/>
<gate name="V39" symbol="VCCIO"/>
<gate name="V40" symbol="VCCIO"/>
<gate name="V41" symbol="VCCIO"/>
<gate name="V42" symbol="VCCIO"/>
<gate name="V43" symbol="VCCIO"/>
<gate name="V44" symbol="VCCIO"/>
<gate name="V45" symbol="VCCIO"/>
<gate name="V46" symbol="VCCIO"/>
<gate name="V47" symbol="VCCIO"/>
<gate name="V48" symbol="VCCIO"/>
<gate name="V49" symbol="VCCIO"/>
<gate name="V50" symbol="VCCIO"/>
<gate name="V51" symbol="VCCIO"/>
<gate name="V52" symbol="VCCIO"/>
<gate name="V53" symbol="VCCIO"/>
<gate name="V54" symbol="VCCIO"/>
<gate name="V55" symbol="VCCIO"/>
<gate name="V56" symbol="VCCIO"/>
<gate name="V57" symbol="VCCIO"/>
<gate name="V58" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="BGA600">
<connects>
<connect gate="-1" pin="IO11" pad="AR6"/>
<connect gate="-1" pin="IO12" pad="AL7"/>
<connect gate="-1" pin="IO13" pad="E7"/>
<connect gate="-1" pin="IO14" pad="A6"/>
<connect gate="-1" pin="IO21" pad="AM7"/>
<connect gate="-1" pin="IO22" pad="AN7"/>
<connect gate="-1" pin="IO23" pad="C7"/>
<connect gate="-1" pin="IO24" pad="D7"/>
<connect gate="-1" pin="IO31" pad="AP7"/>
<connect gate="-1" pin="IO32" pad="AR7"/>
<connect gate="-1" pin="IO33" pad="B7"/>
<connect gate="-1" pin="IO34" pad="A7"/>
<connect gate="-1" pin="IO41" pad="AL8"/>
<connect gate="-1" pin="IO42" pad="AM8"/>
<connect gate="-1" pin="IO43" pad="D8"/>
<connect gate="-1" pin="IO44" pad="E8"/>
<connect gate="-10" pin="IO371" pad="AP23"/>
<connect gate="-10" pin="IO372" pad="AN23"/>
<connect gate="-10" pin="IO373" pad="E23"/>
<connect gate="-10" pin="IO374" pad="D23"/>
<connect gate="-10" pin="IO381" pad="B24"/>
<connect gate="-10" pin="IO382" pad="AM23"/>
<connect gate="-10" pin="IO383" pad="AL23"/>
<connect gate="-10" pin="IO384" pad="A24"/>
<connect gate="-10" pin="IO391" pad="AR24"/>
<connect gate="-10" pin="IO392" pad="AN24"/>
<connect gate="-10" pin="IO393" pad="A25"/>
<connect gate="-10" pin="IO394" pad="C24"/>
<connect gate="-10" pin="IO401" pad="E24"/>
<connect gate="-10" pin="IO402" pad="AM24"/>
<connect gate="-10" pin="IO403" pad="AR25"/>
<connect gate="-10" pin="IO404" pad="B25"/>
<connect gate="-11" pin="IO411" pad="C25"/>
<connect gate="-11" pin="IO412" pad="AL24"/>
<connect gate="-11" pin="IO413" pad="AP25"/>
<connect gate="-11" pin="IO414" pad="D25"/>
<connect gate="-11" pin="IO421" pad="AM25"/>
<connect gate="-11" pin="IO422" pad="AN25"/>
<connect gate="-11" pin="IO423" pad="E25"/>
<connect gate="-11" pin="IO424" pad="A26"/>
<connect gate="-11" pin="IO431" pad="B26"/>
<connect gate="-11" pin="IO432" pad="AR26"/>
<connect gate="-11" pin="IO433" pad="AL25"/>
<connect gate="-11" pin="IO434" pad="C26"/>
<connect gate="-11" pin="IO441" pad="AN26"/>
<connect gate="-11" pin="IO442" pad="AP26"/>
<connect gate="-11" pin="IO443" pad="D26"/>
<connect gate="-11" pin="IO444" pad="E26"/>
<connect gate="-12" pin="IO451" pad="AL26"/>
<connect gate="-12" pin="IO452" pad="AR27"/>
<connect gate="-12" pin="IO453" pad="B27"/>
<connect gate="-12" pin="IO454" pad="C27"/>
<connect gate="-12" pin="IO461" pad="AP27"/>
<connect gate="-12" pin="IO462" pad="AN27"/>
<connect gate="-12" pin="IO463" pad="E27"/>
<connect gate="-12" pin="IO464" pad="D27"/>
<connect gate="-12" pin="IO471" pad="B28"/>
<connect gate="-12" pin="IO472" pad="AM27"/>
<connect gate="-12" pin="IO473" pad="AL27"/>
<connect gate="-12" pin="IO474" pad="A28"/>
<connect gate="-12" pin="IO481" pad="AR28"/>
<connect gate="-12" pin="IO482" pad="AP28"/>
<connect gate="-12" pin="IO483" pad="D28"/>
<connect gate="-12" pin="IO484" pad="C28"/>
<connect gate="-13" pin="IO491" pad="AM28"/>
<connect gate="-13" pin="IO492" pad="AN28"/>
<connect gate="-13" pin="IO493" pad="A29"/>
<connect gate="-13" pin="IO494" pad="E28"/>
<connect gate="-13" pin="IO501" pad="AR29"/>
<connect gate="-13" pin="IO502" pad="AL28"/>
<connect gate="-13" pin="IO503" pad="B29"/>
<connect gate="-13" pin="IO504" pad="C29"/>
<connect gate="-13" pin="IO511" pad="AN29"/>
<connect gate="-13" pin="IO512" pad="AP29"/>
<connect gate="-13" pin="IO513" pad="D29"/>
<connect gate="-13" pin="IO514" pad="E29"/>
<connect gate="-13" pin="IO521" pad="AL29"/>
<connect gate="-13" pin="IO522" pad="AM29"/>
<connect gate="-13" pin="IO523" pad="A30"/>
<connect gate="-13" pin="IO524" pad="B30"/>
<connect gate="-2" pin="IO51" pad="B8"/>
<connect gate="-2" pin="IO52" pad="AR8"/>
<connect gate="-2" pin="IO53" pad="AP8"/>
<connect gate="-2" pin="IO54" pad="A8"/>
<connect gate="-2" pin="IO61" pad="AM9"/>
<connect gate="-2" pin="IO62" pad="AL9"/>
<connect gate="-2" pin="IO63" pad="E9"/>
<connect gate="-2" pin="IO64" pad="D9"/>
<connect gate="-2" pin="IO71" pad="AP9"/>
<connect gate="-2" pin="IO72" pad="AN9"/>
<connect gate="-2" pin="IO73" pad="C9"/>
<connect gate="-2" pin="IO74" pad="B9"/>
<connect gate="-2" pin="IO81" pad="A9"/>
<connect gate="-2" pin="IO82" pad="AL10"/>
<connect gate="-2" pin="IO83" pad="AR9"/>
<connect gate="-2" pin="IO84" pad="E10"/>
<connect gate="-3" pin="IO101" pad="A10"/>
<connect gate="-3" pin="IO102" pad="AP10"/>
<connect gate="-3" pin="IO103" pad="AR10"/>
<connect gate="-3" pin="IO104" pad="B10"/>
<connect gate="-3" pin="IO111" pad="D11"/>
<connect gate="-3" pin="IO112" pad="AL11"/>
<connect gate="-3" pin="IO113" pad="AM11"/>
<connect gate="-3" pin="IO114" pad="E11"/>
<connect gate="-3" pin="IO121" pad="AN11"/>
<connect gate="-3" pin="IO122" pad="AP11"/>
<connect gate="-3" pin="IO123" pad="B11"/>
<connect gate="-3" pin="IO124" pad="C11"/>
<connect gate="-3" pin="IO91" pad="AM10"/>
<connect gate="-3" pin="IO92" pad="AN10"/>
<connect gate="-3" pin="IO93" pad="C10"/>
<connect gate="-3" pin="IO94" pad="D10"/>
<connect gate="-4" pin="IO131" pad="D12"/>
<connect gate="-4" pin="IO132" pad="AN12"/>
<connect gate="-4" pin="IO133" pad="AM12"/>
<connect gate="-4" pin="IO134" pad="C12"/>
<connect gate="-4" pin="IO141" pad="AR12"/>
<connect gate="-4" pin="IO142" pad="AP12"/>
<connect gate="-4" pin="IO143" pad="B12"/>
<connect gate="-4" pin="IO144" pad="A12"/>
<connect gate="-4" pin="IO151" pad="AM13"/>
<connect gate="-4" pin="IO152" pad="AL13"/>
<connect gate="-4" pin="IO153" pad="E13"/>
<connect gate="-4" pin="IO154" pad="D13"/>
<connect gate="-4" pin="IO161" pad="C13"/>
<connect gate="-4" pin="IO162" pad="AP13"/>
<connect gate="-4" pin="IO163" pad="AN13"/>
<connect gate="-4" pin="IO164" pad="B13"/>
<connect gate="-5" pin="IO171" pad="AR13"/>
<connect gate="-5" pin="IO172" pad="AL14"/>
<connect gate="-5" pin="IO173" pad="E14"/>
<connect gate="-5" pin="IO174" pad="A13"/>
<connect gate="-5" pin="IO181" pad="AM14"/>
<connect gate="-5" pin="IO182" pad="AN14"/>
<connect gate="-5" pin="IO183" pad="C14"/>
<connect gate="-5" pin="IO184" pad="D14"/>
<connect gate="-5" pin="IO191" pad="A14"/>
<connect gate="-5" pin="IO192" pad="AP14"/>
<connect gate="-5" pin="IO193" pad="AR14"/>
<connect gate="-5" pin="IO194" pad="B14"/>
<connect gate="-5" pin="IO201" pad="AL15"/>
<connect gate="-5" pin="IO202" pad="AM15"/>
<connect gate="-5" pin="IO203" pad="D15"/>
<connect gate="-5" pin="IO204" pad="E15"/>
<connect gate="-6" pin="IO211" pad="B15"/>
<connect gate="-6" pin="IO212" pad="AR15"/>
<connect gate="-6" pin="IO213" pad="AP15"/>
<connect gate="-6" pin="IO214" pad="A15"/>
<connect gate="-6" pin="IO221" pad="AM16"/>
<connect gate="-6" pin="IO222" pad="AL16"/>
<connect gate="-6" pin="IO223" pad="E16"/>
<connect gate="-6" pin="IO224" pad="D16"/>
<connect gate="-6" pin="IO231" pad="C16"/>
<connect gate="-6" pin="IO232" pad="AP16"/>
<connect gate="-6" pin="IO233" pad="AN16"/>
<connect gate="-6" pin="IO234" pad="B16"/>
<connect gate="-6" pin="IO241" pad="AL17"/>
<connect gate="-6" pin="IO242" pad="AR16"/>
<connect gate="-6" pin="IO243" pad="A16"/>
<connect gate="-6" pin="IO244" pad="E17"/>
<connect gate="-7" pin="IO251" pad="AN17"/>
<connect gate="-7" pin="IO252" pad="AM17"/>
<connect gate="-7" pin="IO253" pad="C17"/>
<connect gate="-7" pin="IO254" pad="D17"/>
<connect gate="-7" pin="IO261" pad="A17"/>
<connect gate="-7" pin="IO262" pad="AP17"/>
<connect gate="-7" pin="IO263" pad="AR17"/>
<connect gate="-7" pin="IO264" pad="B17"/>
<connect gate="-7" pin="IO271" pad="AR19"/>
<connect gate="-7" pin="IO272" pad="AP18"/>
<connect gate="-7" pin="IO273" pad="B19"/>
<connect gate="-7" pin="IO274" pad="C19"/>
<connect gate="-7" pin="IO281" pad="D19"/>
<connect gate="-7" pin="IO282" pad="AP19"/>
<connect gate="-7" pin="IO283" pad="AN19"/>
<connect gate="-7" pin="IO284" pad="E19"/>
<connect gate="-8" pin="IO291" pad="AL19"/>
<connect gate="-8" pin="IO292" pad="AR20"/>
<connect gate="-8" pin="IO293" pad="C20"/>
<connect gate="-8" pin="IO294" pad="B20"/>
<connect gate="-8" pin="IO301" pad="E20"/>
<connect gate="-8" pin="IO302" pad="AP20"/>
<connect gate="-8" pin="IO303" pad="AN20"/>
<connect gate="-8" pin="IO304" pad="D20"/>
<connect gate="-8" pin="IO311" pad="AM20"/>
<connect gate="-8" pin="IO312" pad="AL20"/>
<connect gate="-8" pin="IO313" pad="B21"/>
<connect gate="-8" pin="IO314" pad="A21"/>
<connect gate="-8" pin="IO321" pad="D21"/>
<connect gate="-8" pin="IO322" pad="AR21"/>
<connect gate="-8" pin="IO323" pad="AP21"/>
<connect gate="-8" pin="IO324" pad="C21"/>
<connect gate="-9" pin="IO331" pad="AM21"/>
<connect gate="-9" pin="IO332" pad="AN21"/>
<connect gate="-9" pin="IO333" pad="E21"/>
<connect gate="-9" pin="IO334" pad="A22"/>
<connect gate="-9" pin="IO341" pad="AR22"/>
<connect gate="-9" pin="IO342" pad="AL21"/>
<connect gate="-9" pin="IO343" pad="B22"/>
<connect gate="-9" pin="IO344" pad="C22"/>
<connect gate="-9" pin="IO351" pad="D22"/>
<connect gate="-9" pin="IO352" pad="AN22"/>
<connect gate="-9" pin="IO353" pad="AP22"/>
<connect gate="-9" pin="IO354" pad="E22"/>
<connect gate="-9" pin="IO361" pad="AL22"/>
<connect gate="-9" pin="IO362" pad="AM22"/>
<connect gate="-9" pin="IO363" pad="A23"/>
<connect gate="-9" pin="IO364" pad="B23"/>
<connect gate="-A" pin="IOA1" pad="AL2"/>
<connect gate="-A" pin="IOA10" pad="AK32"/>
<connect gate="-A" pin="IOA11" pad="AJ5"/>
<connect gate="-A" pin="IOA12" pad="AM35"/>
<connect gate="-A" pin="IOA13" pad="AL4"/>
<connect gate="-A" pin="IOA14" pad="AL34"/>
<connect gate="-A" pin="IOA15" pad="AM2"/>
<connect gate="-A" pin="IOA16" pad="AM33"/>
<connect gate="-A" pin="IOA2" pad="AK5"/>
<connect gate="-A" pin="IOA3" pad="AL32"/>
<connect gate="-A" pin="IOA4" pad="AL33"/>
<connect gate="-A" pin="IOA5" pad="AM1"/>
<connect gate="-A" pin="IOA6" pad="AM3"/>
<connect gate="-A" pin="IOA7" pad="AM34"/>
<connect gate="-A" pin="IOA8" pad="AJ31"/>
<connect gate="-A" pin="IOA9" pad="AK4"/>
<connect gate="-B" pin="IOB1" pad="AJ2"/>
<connect gate="-B" pin="IOB10" pad="AK34"/>
<connect gate="-B" pin="IOB11" pad="AK1"/>
<connect gate="-B" pin="IOB12" pad="AH31"/>
<connect gate="-B" pin="IOB13" pad="AH5"/>
<connect gate="-B" pin="IOB14" pad="AK33"/>
<connect gate="-B" pin="IOB15" pad="AJ35"/>
<connect gate="-B" pin="IOB16" pad="AK3"/>
<connect gate="-B" pin="IOB2" pad="AJ33"/>
<connect gate="-B" pin="IOB3" pad="AJ3"/>
<connect gate="-B" pin="IOB4" pad="AJ34"/>
<connect gate="-B" pin="IOB5" pad="AK2"/>
<connect gate="-B" pin="IOB6" pad="AJ4"/>
<connect gate="-B" pin="IOB7" pad="AL1"/>
<connect gate="-B" pin="IOB8" pad="AL35"/>
<connect gate="-B" pin="IOB9" pad="AJ32"/>
<connect gate="-C" pin="IOC1" pad="AG2"/>
<connect gate="-C" pin="IOC10" pad="AH32"/>
<connect gate="-C" pin="IOC11" pad="AG4"/>
<connect gate="-C" pin="IOC12" pad="AH34"/>
<connect gate="-C" pin="IOC13" pad="AH2"/>
<connect gate="-C" pin="IOC14" pad="AG31"/>
<connect gate="-C" pin="IOC15" pad="AG34"/>
<connect gate="-C" pin="IOC16" pad="AH4"/>
<connect gate="-C" pin="IOC2" pad="AG32"/>
<connect gate="-C" pin="IOC3" pad="AG3"/>
<connect gate="-C" pin="IOC4" pad="AG33"/>
<connect gate="-C" pin="IOC5" pad="AH1"/>
<connect gate="-C" pin="IOC6" pad="AH3"/>
<connect gate="-C" pin="IOC7" pad="AH33"/>
<connect gate="-C" pin="IOC8" pad="AH35"/>
<connect gate="-C" pin="IOC9" pad="AJ1"/>
<connect gate="-D" pin="IOD1" pad="AE5"/>
<connect gate="-D" pin="IOD10" pad="AE3"/>
<connect gate="-D" pin="IOD11" pad="AE31"/>
<connect gate="-D" pin="IOD12" pad="AF1"/>
<connect gate="-D" pin="IOD13" pad="AF34"/>
<connect gate="-D" pin="IOD14" pad="AF3"/>
<connect gate="-D" pin="IOD15" pad="AG35"/>
<connect gate="-D" pin="IOD16" pad="AG1"/>
<connect gate="-D" pin="IOD2" pad="AE32"/>
<connect gate="-D" pin="IOD3" pad="AF2"/>
<connect gate="-D" pin="IOD4" pad="AF35"/>
<connect gate="-D" pin="IOD5" pad="AF4"/>
<connect gate="-D" pin="IOD6" pad="AF5"/>
<connect gate="-D" pin="IOD7" pad="AF31"/>
<connect gate="-D" pin="IOD8" pad="AF33"/>
<connect gate="-D" pin="IOD9" pad="AE33"/>
<connect gate="-E" pin="IOE1" pad="AC5"/>
<connect gate="-E" pin="IOE10" pad="AD31"/>
<connect gate="-E" pin="IOE11" pad="AC32"/>
<connect gate="-E" pin="IOE12" pad="AD2"/>
<connect gate="-E" pin="IOE13" pad="AD32"/>
<connect gate="-E" pin="IOE14" pad="AD4"/>
<connect gate="-E" pin="IOE15" pad="AE35"/>
<connect gate="-E" pin="IOE16" pad="AE1"/>
<connect gate="-E" pin="IOE2" pad="AD34"/>
<connect gate="-E" pin="IOE3" pad="AD1"/>
<connect gate="-E" pin="IOE4" pad="AD3"/>
<connect gate="-E" pin="IOE5" pad="AD33"/>
<connect gate="-E" pin="IOE6" pad="AC31"/>
<connect gate="-E" pin="IOE7" pad="AD5"/>
<connect gate="-E" pin="IOE8" pad="AE2"/>
<connect gate="-E" pin="IOE9" pad="AE34"/>
<connect gate="-F" pin="IOF1" pad="AB2"/>
<connect gate="-F" pin="IOF10" pad="AB33"/>
<connect gate="-F" pin="IOF11" pad="AB35"/>
<connect gate="-F" pin="IOF12" pad="AB3"/>
<connect gate="-F" pin="IOF13" pad="AB31"/>
<connect gate="-F" pin="IOF14" pad="AC1"/>
<connect gate="-F" pin="IOF15" pad="AC3"/>
<connect gate="-F" pin="IOF16" pad="AC34"/>
<connect gate="-F" pin="IOF2" pad="AB34"/>
<connect gate="-F" pin="IOF3" pad="AB4"/>
<connect gate="-F" pin="IOF4" pad="AB32"/>
<connect gate="-F" pin="IOF5" pad="AC2"/>
<connect gate="-F" pin="IOF6" pad="AC4"/>
<connect gate="-F" pin="IOF7" pad="AC33"/>
<connect gate="-F" pin="IOF8" pad="AC35"/>
<connect gate="-F" pin="IOF9" pad="AB1"/>
<connect gate="-G" pin="IOG1" pad="Y4"/>
<connect gate="-G" pin="IOG10" pad="Y31"/>
<connect gate="-G" pin="IOG11" pad="Y32"/>
<connect gate="-G" pin="IOG12" pad="Y5"/>
<connect gate="-G" pin="IOG13" pad="AA35"/>
<connect gate="-G" pin="IOG14" pad="AA2"/>
<connect gate="-G" pin="IOG15" pad="AA32"/>
<connect gate="-G" pin="IOG16" pad="AA4"/>
<connect gate="-G" pin="IOG2" pad="Y33"/>
<connect gate="-G" pin="IOG3" pad="AA3"/>
<connect gate="-G" pin="IOG4" pad="AA34"/>
<connect gate="-G" pin="IOG5" pad="Y34"/>
<connect gate="-G" pin="IOG6" pad="Y3"/>
<connect gate="-G" pin="IOG7" pad="AA1"/>
<connect gate="-G" pin="IOG8" pad="AA5"/>
<connect gate="-G" pin="IOG9" pad="AA31"/>
<connect gate="-H" pin="IOH1" pad="V33"/>
<connect gate="-H" pin="IOH10" pad="W3"/>
<connect gate="-H" pin="IOH11" pad="W4"/>
<connect gate="-H" pin="IOH12" pad="Y1"/>
<connect gate="-H" pin="IOH13" pad="Y35"/>
<connect gate="-H" pin="IOH14" pad="W32"/>
<connect gate="-H" pin="IOH15" pad="W31"/>
<connect gate="-H" pin="IOH16" pad="W5"/>
<connect gate="-H" pin="IOH2" pad="V4"/>
<connect gate="-H" pin="IOH3" pad="W1"/>
<connect gate="-H" pin="IOH4" pad="V5"/>
<connect gate="-H" pin="IOH5" pad="W2"/>
<connect gate="-H" pin="IOH6" pad="W34"/>
<connect gate="-H" pin="IOH7" pad="V31"/>
<connect gate="-H" pin="IOH8" pad="W33"/>
<connect gate="-H" pin="IOH9" pad="W35"/>
<connect gate="-I" pin="IOI1" pad="T31"/>
<connect gate="-I" pin="IOI10" pad="U33"/>
<connect gate="-I" pin="IOI11" pad="U31"/>
<connect gate="-I" pin="IOI12" pad="V35"/>
<connect gate="-I" pin="IOI13" pad="U32"/>
<connect gate="-I" pin="IOI14" pad="V2"/>
<connect gate="-I" pin="IOI15" pad="V3"/>
<connect gate="-I" pin="IOI16" pad="V34"/>
<connect gate="-I" pin="IOI2" pad="T5"/>
<connect gate="-I" pin="IOI3" pad="U1"/>
<connect gate="-I" pin="IOI4" pad="U35"/>
<connect gate="-I" pin="IOI5" pad="U34"/>
<connect gate="-I" pin="IOI6" pad="U2"/>
<connect gate="-I" pin="IOI7" pad="U5"/>
<connect gate="-I" pin="IOI8" pad="V1"/>
<connect gate="-I" pin="IOI9" pad="U4"/>
<connect gate="-J" pin="IOJ1" pad="T3"/>
<connect gate="-J" pin="IOJ10" pad="R33"/>
<connect gate="-J" pin="IOJ11" pad="R4"/>
<connect gate="-J" pin="IOJ12" pad="R31"/>
<connect gate="-J" pin="IOJ13" pad="T1"/>
<connect gate="-J" pin="IOJ14" pad="R3"/>
<connect gate="-J" pin="IOJ15" pad="R34"/>
<connect gate="-J" pin="IOJ16" pad="T33"/>
<connect gate="-J" pin="IOJ2" pad="R5"/>
<connect gate="-J" pin="IOJ3" pad="R32"/>
<connect gate="-J" pin="IOJ4" pad="T2"/>
<connect gate="-J" pin="IOJ5" pad="T4"/>
<connect gate="-J" pin="IOJ6" pad="T32"/>
<connect gate="-J" pin="IOJ7" pad="T34"/>
<connect gate="-J" pin="IOJ8" pad="R35"/>
<connect gate="-J" pin="IOJ9" pad="R2"/>
<connect gate="-K" pin="IOK1" pad="N33"/>
<connect gate="-K" pin="IOK10" pad="N32"/>
<connect gate="-K" pin="IOK11" pad="P1"/>
<connect gate="-K" pin="IOK12" pad="P35"/>
<connect gate="-K" pin="IOK13" pad="P3"/>
<connect gate="-K" pin="IOK14" pad="R1"/>
<connect gate="-K" pin="IOK15" pad="P31"/>
<connect gate="-K" pin="IOK16" pad="P33"/>
<connect gate="-K" pin="IOK2" pad="N5"/>
<connect gate="-K" pin="IOK3" pad="P34"/>
<connect gate="-K" pin="IOK4" pad="P4"/>
<connect gate="-K" pin="IOK5" pad="P2"/>
<connect gate="-K" pin="IOK6" pad="P32"/>
<connect gate="-K" pin="IOK7" pad="N4"/>
<connect gate="-K" pin="IOK8" pad="N3"/>
<connect gate="-K" pin="IOK9" pad="N31"/>
<connect gate="-L" pin="IOL1" pad="L34"/>
<connect gate="-L" pin="IOL10" pad="L35"/>
<connect gate="-L" pin="IOL11" pad="M1"/>
<connect gate="-L" pin="IOL12" pad="M4"/>
<connect gate="-L" pin="IOL13" pad="M33"/>
<connect gate="-L" pin="IOL14" pad="M31"/>
<connect gate="-L" pin="IOL15" pad="N2"/>
<connect gate="-L" pin="IOL16" pad="N35"/>
<connect gate="-L" pin="IOL2" pad="L2"/>
<connect gate="-L" pin="IOL3" pad="M34"/>
<connect gate="-L" pin="IOL4" pad="M3"/>
<connect gate="-L" pin="IOL5" pad="M32"/>
<connect gate="-L" pin="IOL6" pad="N1"/>
<connect gate="-L" pin="IOL7" pad="M5"/>
<connect gate="-L" pin="IOL8" pad="M35"/>
<connect gate="-L" pin="IOL9" pad="L1"/>
<connect gate="-M" pin="IOM1" pad="K31"/>
<connect gate="-M" pin="IOM10" pad="J35"/>
<connect gate="-M" pin="IOM11" pad="K2"/>
<connect gate="-M" pin="IOM12" pad="K34"/>
<connect gate="-M" pin="IOM13" pad="L3"/>
<connect gate="-M" pin="IOM14" pad="L4"/>
<connect gate="-M" pin="IOM15" pad="L32"/>
<connect gate="-M" pin="IOM16" pad="L33"/>
<connect gate="-M" pin="IOM2" pad="K3"/>
<connect gate="-M" pin="IOM3" pad="K35"/>
<connect gate="-M" pin="IOM4" pad="K1"/>
<connect gate="-M" pin="IOM5" pad="L31"/>
<connect gate="-M" pin="IOM6" pad="L5"/>
<connect gate="-M" pin="IOM7" pad="K4"/>
<connect gate="-M" pin="IOM8" pad="J1"/>
<connect gate="-M" pin="IOM9" pad="K33"/>
<connect gate="-N" pin="ION1" pad="H4"/>
<connect gate="-N" pin="ION10" pad="H32"/>
<connect gate="-N" pin="ION11" pad="J31"/>
<connect gate="-N" pin="ION12" pad="H34"/>
<connect gate="-N" pin="ION13" pad="J3"/>
<connect gate="-N" pin="ION14" pad="J32"/>
<connect gate="-N" pin="ION15" pad="K5"/>
<connect gate="-N" pin="ION16" pad="J34"/>
<connect gate="-N" pin="ION2" pad="H33"/>
<connect gate="-N" pin="ION3" pad="H3"/>
<connect gate="-N" pin="ION4" pad="H35"/>
<connect gate="-N" pin="ION5" pad="J2"/>
<connect gate="-N" pin="ION6" pad="J4"/>
<connect gate="-N" pin="ION7" pad="J33"/>
<connect gate="-N" pin="ION8" pad="H2"/>
<connect gate="-N" pin="ION9" pad="J5"/>
<connect gate="-O" pin="IOO1" pad="F3"/>
<connect gate="-O" pin="IOO10" pad="F33"/>
<connect gate="-O" pin="IOO11" pad="H31"/>
<connect gate="-O" pin="IOO12" pad="G1"/>
<connect gate="-O" pin="IOO13" pad="G3"/>
<connect gate="-O" pin="IOO14" pad="G33"/>
<connect gate="-O" pin="IOO15" pad="G35"/>
<connect gate="-O" pin="IOO16" pad="G2"/>
<connect gate="-O" pin="IOO2" pad="E35"/>
<connect gate="-O" pin="IOO3" pad="G32"/>
<connect gate="-O" pin="IOO4" pad="H5"/>
<connect gate="-O" pin="IOO5" pad="F34"/>
<connect gate="-O" pin="IOO6" pad="F1"/>
<connect gate="-O" pin="IOO7" pad="G34"/>
<connect gate="-O" pin="IOO8" pad="F2"/>
<connect gate="-O" pin="IOO9" pad="G4"/>
<connect gate="-P" pin="IOP1" pad="E4"/>
<connect gate="-P" pin="IOP10" pad="D3"/>
<connect gate="-P" pin="IOP11" pad="D35"/>
<connect gate="-P" pin="IOP12" pad="F4"/>
<connect gate="-P" pin="IOP13" pad="D33"/>
<connect gate="-P" pin="IOP14" pad="F32"/>
<connect gate="-P" pin="IOP15" pad="E1"/>
<connect gate="-P" pin="IOP16" pad="E34"/>
<connect gate="-P" pin="IOP2" pad="E32"/>
<connect gate="-P" pin="IOP3" pad="D34"/>
<connect gate="-P" pin="IOP4" pad="G5"/>
<connect gate="-P" pin="IOP5" pad="D2"/>
<connect gate="-P" pin="IOP6" pad="G31"/>
<connect gate="-P" pin="IOP7" pad="E33"/>
<connect gate="-P" pin="IOP8" pad="E3"/>
<connect gate="-P" pin="IOP9" pad="D1"/>
<connect gate="G1" pin="GND" pad="AL6"/>
<connect gate="G10" pin="GND" pad="AP2"/>
<connect gate="G11" pin="GND" pad="AP3"/>
<connect gate="G12" pin="GND" pad="AP4"/>
<connect gate="G13" pin="GND" pad="AP5"/>
<connect gate="G14" pin="GND" pad="AP6"/>
<connect gate="G15" pin="GND" pad="AP30"/>
<connect gate="G16" pin="GND" pad="AP31"/>
<connect gate="G17" pin="GND" pad="AP32"/>
<connect gate="G18" pin="GND" pad="AP33"/>
<connect gate="G19" pin="GND" pad="AR1"/>
<connect gate="G2" pin="GND" pad="AL30"/>
<connect gate="G20" pin="GND" pad="AR2"/>
<connect gate="G21" pin="GND" pad="AR3"/>
<connect gate="G22" pin="GND" pad="AR4"/>
<connect gate="G23" pin="GND" pad="AR5"/>
<connect gate="G24" pin="GND" pad="AR30"/>
<connect gate="G25" pin="GND" pad="AR31"/>
<connect gate="G26" pin="GND" pad="AR32"/>
<connect gate="G27" pin="GND" pad="AR33"/>
<connect gate="G28" pin="GND" pad="AR34"/>
<connect gate="G29" pin="GND" pad="AR35"/>
<connect gate="G3" pin="GND" pad="AM6"/>
<connect gate="G30" pin="GND" pad="A1"/>
<connect gate="G31" pin="GND" pad="A2"/>
<connect gate="G32" pin="GND" pad="A3"/>
<connect gate="G33" pin="GND" pad="A4"/>
<connect gate="G34" pin="GND" pad="A5"/>
<connect gate="G35" pin="GND" pad="A18"/>
<connect gate="G36" pin="GND" pad="A31"/>
<connect gate="G37" pin="GND" pad="A32"/>
<connect gate="G38" pin="GND" pad="A33"/>
<connect gate="G39" pin="GND" pad="A34"/>
<connect gate="G4" pin="GND" pad="AM30"/>
<connect gate="G40" pin="GND" pad="A35"/>
<connect gate="G41" pin="GND" pad="B2"/>
<connect gate="G42" pin="GND" pad="B3"/>
<connect gate="G43" pin="GND" pad="B4"/>
<connect gate="G44" pin="GND" pad="B5"/>
<connect gate="G45" pin="GND" pad="B6"/>
<connect gate="G46" pin="GND" pad="B31"/>
<connect gate="G47" pin="GND" pad="B32"/>
<connect gate="G48" pin="GND" pad="B33"/>
<connect gate="G49" pin="GND" pad="B34"/>
<connect gate="G5" pin="GND" pad="AN5"/>
<connect gate="G50" pin="GND" pad="B35"/>
<connect gate="G51" pin="GND" pad="C5"/>
<connect gate="G52" pin="GND" pad="C6"/>
<connect gate="G53" pin="GND" pad="C30"/>
<connect gate="G54" pin="GND" pad="C31"/>
<connect gate="G55" pin="GND" pad="D6"/>
<connect gate="G56" pin="GND" pad="D30"/>
<connect gate="G57" pin="GND" pad="E6"/>
<connect gate="G58" pin="GND" pad="E30"/>
<connect gate="G6" pin="GND" pad="AN6"/>
<connect gate="G7" pin="GND" pad="AN30"/>
<connect gate="G8" pin="GND" pad="AN31"/>
<connect gate="G9" pin="GND" pad="AN35"/>
<connect gate="V1" pin="VCC" pad="AA33"/>
<connect gate="V10" pin="VCC" pad="AP24"/>
<connect gate="V11" pin="VCC" pad="AR11"/>
<connect gate="V12" pin="VCC" pad="AR18"/>
<connect gate="V13" pin="VCC" pad="A11"/>
<connect gate="V14" pin="VCC" pad="A19"/>
<connect gate="V15" pin="VCC" pad="B1"/>
<connect gate="V16" pin="VCC" pad="B18"/>
<connect gate="V17" pin="VCC" pad="D24"/>
<connect gate="V18" pin="VCC" pad="E2"/>
<connect gate="V19" pin="VCC" pad="F31"/>
<connect gate="V2" pin="VCC" pad="AB5"/>
<connect gate="V20" pin="VCC" pad="F35"/>
<connect gate="V21" pin="VCC" pad="H1"/>
<connect gate="V22" pin="VCC" pad="K32"/>
<connect gate="V23" pin="VCC" pad="M2"/>
<connect gate="V24" pin="VCC" pad="N34"/>
<connect gate="V25" pin="VCC" pad="P5"/>
<connect gate="V26" pin="VCC" pad="T35"/>
<connect gate="V27" pin="VCC" pad="U3"/>
<connect gate="V28" pin="VCC" pad="V32"/>
<connect gate="V29" pin="VCC" pad="Y2"/>
<connect gate="V3" pin="VCC" pad="AD35"/>
<connect gate="V30" pin="VCCIO" pad="AL5"/>
<connect gate="V31" pin="VCCIO" pad="AL12"/>
<connect gate="V32" pin="VCCIO" pad="AM5"/>
<connect gate="V33" pin="VCCIO" pad="AM19"/>
<connect gate="V34" pin="VCCIO" pad="AM26"/>
<connect gate="V35" pin="VCCIO" pad="AM31"/>
<connect gate="V36" pin="VCCIO" pad="AN3"/>
<connect gate="V37" pin="VCCIO" pad="AN4"/>
<connect gate="V38" pin="VCCIO" pad="AN8"/>
<connect gate="V39" pin="VCCIO" pad="AN15"/>
<connect gate="V4" pin="VCC" pad="AE4"/>
<connect gate="V40" pin="VCCIO" pad="AN32"/>
<connect gate="V41" pin="VCCIO" pad="AN33"/>
<connect gate="V42" pin="VCCIO" pad="AP34"/>
<connect gate="V43" pin="VCCIO" pad="AR23"/>
<connect gate="V44" pin="VCCIO" pad="A20"/>
<connect gate="V45" pin="VCCIO" pad="A27"/>
<connect gate="V46" pin="VCCIO" pad="C2"/>
<connect gate="V47" pin="VCCIO" pad="C3"/>
<connect gate="V48" pin="VCCIO" pad="C4"/>
<connect gate="V49" pin="VCCIO" pad="C8"/>
<connect gate="V5" pin="VCC" pad="AF32"/>
<connect gate="V50" pin="VCCIO" pad="C15"/>
<connect gate="V51" pin="VCCIO" pad="C23"/>
<connect gate="V52" pin="VCCIO" pad="C32"/>
<connect gate="V53" pin="VCCIO" pad="C33"/>
<connect gate="V54" pin="VCCIO" pad="D5"/>
<connect gate="V55" pin="VCCIO" pad="D31"/>
<connect gate="V56" pin="VCCIO" pad="E5"/>
<connect gate="V57" pin="VCCIO" pad="E12"/>
<connect gate="V58" pin="VCCIO" pad="E31"/>
<connect gate="V6" pin="VCC" pad="AG5"/>
<connect gate="V7" pin="VCC" pad="AK31"/>
<connect gate="V8" pin="VCC" pad="AK35"/>
<connect gate="V9" pin="VCC" pad="AL3"/>
<connect gate="_" pin="/CE" pad="AN2"/>
<connect gate="_" pin="/CEO" pad="AP35"/>
<connect gate="_" pin="/CONFIG" pad="D4"/>
<connect gate="_" pin="/STATUS" pad="D32"/>
<connect gate="_" pin="CONF_DONE" pad="AM32"/>
<connect gate="_" pin="DATA0" pad="AM4"/>
<connect gate="_" pin="DCLK" pad="AP1"/>
<connect gate="_" pin="GCLK0" pad="E18"/>
<connect gate="_" pin="GCLK1" pad="AL18"/>
<connect gate="_" pin="IN0" pad="AN18"/>
<connect gate="_" pin="IN1" pad="AM18"/>
<connect gate="_" pin="IN2" pad="C18"/>
<connect gate="_" pin="IN3" pad="D18"/>
<connect gate="_" pin="MSEL0" pad="F5"/>
<connect gate="_" pin="MSEL1" pad="C1"/>
<connect gate="_" pin="TCK" pad="AL31"/>
<connect gate="_" pin="TDI" pad="AN1"/>
<connect gate="_" pin="TDO" pad="AN34"/>
<connect gate="_" pin="TMS" pad="C35"/>
<connect gate="_" pin="TRST" pad="C34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K130-FPGA484" prefix="IC">
<description>&lt;b&gt;EPF10K130&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="130E484C"/>
<gate name="-A" symbol="A12-484"/>
<gate name="-B" symbol="B12-484"/>
<gate name="-C" symbol="C12-484"/>
<gate name="-D" symbol="D12-484"/>
<gate name="-E" symbol="E11-484"/>
<gate name="-F" symbol="F12-484"/>
<gate name="-G" symbol="G10-484"/>
<gate name="-H" symbol="H10-484"/>
<gate name="-I" symbol="I10-484"/>
<gate name="-J" symbol="J10-484"/>
<gate name="-K" symbol="K11-484"/>
<gate name="-L" symbol="L10-484"/>
<gate name="-M" symbol="M12-484"/>
<gate name="-N" symbol="N11-484"/>
<gate name="-O" symbol="O12-484"/>
<gate name="-P" symbol="P12-484"/>
<gate name="-1" symbol="51-484"/>
<gate name="-2" symbol="93-484"/>
<gate name="-3" symbol="141-484"/>
<gate name="-4" symbol="181-484"/>
<gate name="-5" symbol="222-484"/>
<gate name="-6" symbol="263-484"/>
<gate name="-7" symbol="311-484"/>
<gate name="-8" symbol="354-484"/>
<gate name="-9" symbol="403-484"/>
<gate name="-10" symbol="451-484"/>
<gate name="-11" symbol="493-484"/>
<gate name="-12" symbol="524-484"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCINT"/>
<gate name="14" symbol="VCCINT"/>
<gate name="15" symbol="VCCINT"/>
<gate name="16" symbol="VCCINT"/>
<gate name="17" symbol="VCCINT"/>
<gate name="18" symbol="VCCINT"/>
<gate name="19" symbol="VCCINT"/>
<gate name="20" symbol="VCCINT"/>
<gate name="21" symbol="VCCINT"/>
<gate name="22" symbol="VCCINT"/>
<gate name="23" symbol="VCCINT"/>
<gate name="24" symbol="VCCIO"/>
<gate name="25" symbol="VCCIO"/>
<gate name="26" symbol="VCCIO"/>
<gate name="27" symbol="VCCIO"/>
<gate name="28" symbol="VCCIO"/>
<gate name="29" symbol="VCCIO"/>
<gate name="30" symbol="VCCIO"/>
<gate name="31" symbol="VCCIO"/>
<gate name="32" symbol="VCCIO"/>
<gate name="33" symbol="VCCIO"/>
<gate name="34" symbol="VCCIO"/>
<gate name="35" symbol="VCCIO"/>
<gate name="36" symbol="VCCIO"/>
<gate name="37" symbol="VCCIO"/>
<gate name="38" symbol="VCCIO"/>
<gate name="39" symbol="VCCIO"/>
<gate name="40" symbol="VCCIO"/>
<gate name="41" symbol="VCCIO"/>
<gate name="42" symbol="VCCIO"/>
<gate name="43" symbol="VCCIO"/>
<gate name="44" symbol="VCCIO"/>
<gate name="45" symbol="VCCIO"/>
<gate name="46" symbol="VCCIO"/>
<gate name="47" symbol="VCCIO"/>
<gate name="48" symbol="VCCIO"/>
<gate name="49" symbol="VCCIO"/>
<gate name="50" symbol="VCCIO"/>
<gate name="51" symbol="VCCIO"/>
<gate name="52" symbol="VCCIO"/>
<gate name="53" symbol="GND"/>
<gate name="54" symbol="GND"/>
<gate name="55" symbol="GND"/>
<gate name="56" symbol="GND"/>
<gate name="57" symbol="GND"/>
<gate name="58" symbol="GND"/>
<gate name="59" symbol="GND"/>
<gate name="60" symbol="GND"/>
<gate name="61" symbol="GND"/>
<gate name="62" symbol="GND"/>
<gate name="63" symbol="GND"/>
<gate name="64" symbol="GND"/>
<gate name="65" symbol="GND"/>
<gate name="66" symbol="GND"/>
<gate name="67" symbol="GND"/>
<gate name="68" symbol="GND"/>
<gate name="69" symbol="GND"/>
<gate name="70" symbol="GND"/>
<gate name="71" symbol="GND"/>
<gate name="72" symbol="GND"/>
<gate name="73" symbol="GND"/>
<gate name="74" symbol="GND"/>
<gate name="75" symbol="GND"/>
<gate name="76" symbol="GND"/>
<gate name="77" symbol="GND"/>
<gate name="78" symbol="GND"/>
<gate name="79" symbol="GND"/>
<gate name="80" symbol="GND"/>
<gate name="81" symbol="GND"/>
<gate name="82" symbol="GND"/>
<gate name="83" symbol="GND"/>
<gate name="84" symbol="GND"/>
<gate name="85" symbol="GND"/>
<gate name="86" symbol="GND"/>
<gate name="87" symbol="GND"/>
<gate name="88" symbol="GND"/>
<gate name="89" symbol="GND"/>
<gate name="90" symbol="GND"/>
<gate name="91" symbol="GND"/>
<gate name="92" symbol="GND"/>
<gate name="93" symbol="GND"/>
<gate name="94" symbol="GND"/>
<gate name="95" symbol="GND"/>
<gate name="96" symbol="GND"/>
<gate name="97" symbol="GND"/>
<gate name="98" symbol="GND"/>
<gate name="99" symbol="GND"/>
<gate name="100" symbol="GND"/>
<gate name="101" symbol="GND"/>
</gates>
<devices>
<device name="" package="FBGA484">
<connects>
<connect gate="-1" pin="IO11" pad="AB1"/>
<connect gate="-1" pin="IO12" pad="B3"/>
<connect gate="-1" pin="IO13" pad="C4"/>
<connect gate="-1" pin="IO14" pad="Y4"/>
<connect gate="-1" pin="IO21" pad="AA3"/>
<connect gate="-1" pin="IO22" pad="AA2"/>
<connect gate="-1" pin="IO23" pad="A3"/>
<connect gate="-1" pin="IO24" pad="B4"/>
<connect gate="-1" pin="IO31" pad="AB2"/>
<connect gate="-1" pin="IO32" pad="AA4"/>
<connect gate="-1" pin="IO33" pad="F7"/>
<connect gate="-1" pin="IO34" pad="G8"/>
<connect gate="-1" pin="IO41" pad="AB3"/>
<connect gate="-1" pin="IO42" pad="A4"/>
<connect gate="-1" pin="IO43" pad="W5"/>
<connect gate="-1" pin="IO51" pad="AB4"/>
<connect gate="-10" pin="IO411" pad="G14"/>
<connect gate="-10" pin="IO412" pad="AB17"/>
<connect gate="-10" pin="IO413" pad="D15"/>
<connect gate="-10" pin="IO414" pad="Y16"/>
<connect gate="-10" pin="IO421" pad="T14"/>
<connect gate="-10" pin="IO422" pad="A17"/>
<connect gate="-10" pin="IO423" pad="D16"/>
<connect gate="-10" pin="IO431" pad="AA17"/>
<connect gate="-10" pin="IO432" pad="E15"/>
<connect gate="-10" pin="IO433" pad="C16"/>
<connect gate="-10" pin="IO434" pad="W16"/>
<connect gate="-10" pin="IO441" pad="E16"/>
<connect gate="-10" pin="IO442" pad="AB18"/>
<connect gate="-10" pin="IO443" pad="F15"/>
<connect gate="-10" pin="IO444" pad="V16"/>
<connect gate="-10" pin="IO451" pad="U16"/>
<connect gate="-11" pin="IO452" pad="F16"/>
<connect gate="-11" pin="IO453" pad="C17"/>
<connect gate="-11" pin="IO454" pad="Y17"/>
<connect gate="-11" pin="IO461" pad="AA18"/>
<connect gate="-11" pin="IO462" pad="B18"/>
<connect gate="-11" pin="IO463" pad="A18"/>
<connect gate="-11" pin="IO471" pad="A19"/>
<connect gate="-11" pin="IO472" pad="AB19"/>
<connect gate="-11" pin="IO473" pad="D17"/>
<connect gate="-11" pin="IO474" pad="U17"/>
<connect gate="-11" pin="IO481" pad="Y18"/>
<connect gate="-11" pin="IO482" pad="C18"/>
<connect gate="-11" pin="IO483" pad="W17"/>
<connect gate="-11" pin="IO491" pad="AA19"/>
<connect gate="-11" pin="IO492" pad="F17"/>
<connect gate="-11" pin="IO493" pad="B19"/>
<connect gate="-12" pin="IO494" pad="V17"/>
<connect gate="-12" pin="IO501" pad="C19"/>
<connect gate="-12" pin="IO502" pad="E17"/>
<connect gate="-12" pin="IO503" pad="AB20"/>
<connect gate="-12" pin="IO504" pad="W18"/>
<connect gate="-12" pin="IO511" pad="AA20"/>
<connect gate="-12" pin="IO512" pad="D18"/>
<connect gate="-12" pin="IO513" pad="A20"/>
<connect gate="-12" pin="IO514" pad="Y19"/>
<connect gate="-12" pin="IO521" pad="Y20"/>
<connect gate="-12" pin="IO522" pad="D19"/>
<connect gate="-12" pin="IO523" pad="AB21"/>
<connect gate="-12" pin="IO524" pad="B20"/>
<connect gate="-2" pin="IO52" pad="C5"/>
<connect gate="-2" pin="IO53" pad="G9"/>
<connect gate="-2" pin="IO61" pad="AA5"/>
<connect gate="-2" pin="IO62" pad="D6"/>
<connect gate="-2" pin="IO63" pad="Y5"/>
<connect gate="-2" pin="IO71" pad="W6"/>
<connect gate="-2" pin="IO72" pad="B6"/>
<connect gate="-2" pin="IO73" pad="C6"/>
<connect gate="-2" pin="IO74" pad="V6"/>
<connect gate="-2" pin="IO81" pad="Y6"/>
<connect gate="-2" pin="IO82" pad="AB5"/>
<connect gate="-2" pin="IO83" pad="A5"/>
<connect gate="-2" pin="IO84" pad="F8"/>
<connect gate="-2" pin="IO91" pad="V7"/>
<connect gate="-2" pin="IO92" pad="E6"/>
<connect gate="-2" pin="IO93" pad="C7"/>
<connect gate="-3" pin="IO101" pad="W7"/>
<connect gate="-3" pin="IO102" pad="D5"/>
<connect gate="-3" pin="IO103" pad="A7"/>
<connect gate="-3" pin="IO104" pad="Y7"/>
<connect gate="-3" pin="IO111" pad="T8"/>
<connect gate="-3" pin="IO112" pad="F6"/>
<connect gate="-3" pin="IO113" pad="U8"/>
<connect gate="-3" pin="IO121" pad="AB6"/>
<connect gate="-3" pin="IO122" pad="B7"/>
<connect gate="-3" pin="IO123" pad="E7"/>
<connect gate="-3" pin="IO124" pad="V8"/>
<connect gate="-3" pin="IO131" pad="W8"/>
<connect gate="-3" pin="IO132" pad="D7"/>
<connect gate="-3" pin="IO133" pad="C8"/>
<connect gate="-3" pin="IO141" pad="AB7"/>
<connect gate="-3" pin="IO94" pad="U7"/>
<connect gate="-4" pin="IO142" pad="D8"/>
<connect gate="-4" pin="IO143" pad="G7"/>
<connect gate="-4" pin="IO144" pad="AA7"/>
<connect gate="-4" pin="IO151" pad="R10"/>
<connect gate="-4" pin="IO152" pad="E8"/>
<connect gate="-4" pin="IO153" pad="B8"/>
<connect gate="-4" pin="IO154" pad="T9"/>
<connect gate="-4" pin="IO161" pad="W9"/>
<connect gate="-4" pin="IO162" pad="F9"/>
<connect gate="-4" pin="IO163" pad="E9"/>
<connect gate="-4" pin="IO164" pad="AA8"/>
<connect gate="-4" pin="IO171" pad="D9"/>
<connect gate="-4" pin="IO172" pad="AB8"/>
<connect gate="-4" pin="IO173" pad="C9"/>
<connect gate="-4" pin="IO174" pad="V9"/>
<connect gate="-4" pin="IO181" pad="U9"/>
<connect gate="-5" pin="IO182" pad="A9"/>
<connect gate="-5" pin="IO183" pad="H10"/>
<connect gate="-5" pin="IO184" pad="Y9"/>
<connect gate="-5" pin="IO191" pad="AA9"/>
<connect gate="-5" pin="IO192" pad="B9"/>
<connect gate="-5" pin="IO193" pad="F10"/>
<connect gate="-5" pin="IO201" pad="AB9"/>
<connect gate="-5" pin="IO202" pad="H12"/>
<connect gate="-5" pin="IO203" pad="G10"/>
<connect gate="-5" pin="IO204" pad="T10"/>
<connect gate="-5" pin="IO211" pad="V10"/>
<connect gate="-5" pin="IO212" pad="A10"/>
<connect gate="-5" pin="IO213" pad="D10"/>
<connect gate="-5" pin="IO214" pad="U10"/>
<connect gate="-5" pin="IO221" pad="C10"/>
<connect gate="-5" pin="IO222" pad="B10"/>
<connect gate="-6" pin="IO223" pad="W10"/>
<connect gate="-6" pin="IO224" pad="Y10"/>
<connect gate="-6" pin="IO231" pad="AB10"/>
<connect gate="-6" pin="IO232" pad="E10"/>
<connect gate="-6" pin="IO233" pad="F11"/>
<connect gate="-6" pin="IO234" pad="AA10"/>
<connect gate="-6" pin="IO241" pad="T11"/>
<connect gate="-6" pin="IO242" pad="E11"/>
<connect gate="-6" pin="IO243" pad="G12"/>
<connect gate="-6" pin="IO244" pad="R11"/>
<connect gate="-6" pin="IO251" pad="Y11"/>
<connect gate="-6" pin="IO252" pad="A11"/>
<connect gate="-6" pin="IO253" pad="D11"/>
<connect gate="-6" pin="IO254" pad="U11"/>
<connect gate="-6" pin="IO262" pad="B11"/>
<connect gate="-6" pin="IO263" pad="G11"/>
<connect gate="-7" pin="IO264" pad="AA11"/>
<connect gate="-7" pin="IO271" pad="W12"/>
<connect gate="-7" pin="IO272" pad="AB12"/>
<connect gate="-7" pin="IO273" pad="F12"/>
<connect gate="-7" pin="IO274" pad="A12"/>
<connect gate="-7" pin="IO281" pad="V12"/>
<connect gate="-7" pin="IO282" pad="B12"/>
<connect gate="-7" pin="IO283" pad="C12"/>
<connect gate="-7" pin="IO284" pad="Y12"/>
<connect gate="-7" pin="IO291" pad="AA13"/>
<connect gate="-7" pin="IO292" pad="U12"/>
<connect gate="-7" pin="IO293" pad="B13"/>
<connect gate="-7" pin="IO301" pad="R13"/>
<connect gate="-7" pin="IO302" pad="D13"/>
<connect gate="-7" pin="IO303" pad="T12"/>
<connect gate="-7" pin="IO311" pad="V13"/>
<connect gate="-8" pin="IO312" pad="C13"/>
<connect gate="-8" pin="IO313" pad="E13"/>
<connect gate="-8" pin="IO314" pad="Y13"/>
<connect gate="-8" pin="IO321" pad="AB14"/>
<connect gate="-8" pin="IO322" pad="A14"/>
<connect gate="-8" pin="IO323" pad="W13"/>
<connect gate="-8" pin="IO331" pad="T13"/>
<connect gate="-8" pin="IO332" pad="U13"/>
<connect gate="-8" pin="IO333" pad="B14"/>
<connect gate="-8" pin="IO341" pad="V14"/>
<connect gate="-8" pin="IO342" pad="AA14"/>
<connect gate="-8" pin="IO343" pad="F13"/>
<connect gate="-8" pin="IO351" pad="W14"/>
<connect gate="-8" pin="IO352" pad="C14"/>
<connect gate="-8" pin="IO353" pad="G13"/>
<connect gate="-8" pin="IO354" pad="Y14"/>
<connect gate="-9" pin="IO361" pad="U15"/>
<connect gate="-9" pin="IO362" pad="A15"/>
<connect gate="-9" pin="IO363" pad="H13"/>
<connect gate="-9" pin="IO364" pad="AB15"/>
<connect gate="-9" pin="IO371" pad="B15"/>
<connect gate="-9" pin="IO372" pad="AA15"/>
<connect gate="-9" pin="IO373" pad="D14"/>
<connect gate="-9" pin="IO374" pad="U14"/>
<connect gate="-9" pin="IO381" pad="Y15"/>
<connect gate="-9" pin="IO382" pad="F14"/>
<connect gate="-9" pin="IO383" pad="E14"/>
<connect gate="-9" pin="IO391" pad="A16"/>
<connect gate="-9" pin="IO392" pad="W15"/>
<connect gate="-9" pin="IO401" pad="V15"/>
<connect gate="-9" pin="IO402" pad="AA16"/>
<connect gate="-9" pin="IO403" pad="B16"/>
<connect gate="-A" pin="IOA1" pad="A21"/>
<connect gate="-A" pin="IOA10" pad="D3"/>
<connect gate="-A" pin="IOA11" pad="E3"/>
<connect gate="-A" pin="IOA12" pad="E20"/>
<connect gate="-A" pin="IOA2" pad="C22"/>
<connect gate="-A" pin="IOA3" pad="D20"/>
<connect gate="-A" pin="IOA4" pad="C20"/>
<connect gate="-A" pin="IOA5" pad="G18"/>
<connect gate="-A" pin="IOA6" pad="D2"/>
<connect gate="-A" pin="IOA7" pad="A2"/>
<connect gate="-A" pin="IOA8" pad="C1"/>
<connect gate="-A" pin="IOA9" pad="C3"/>
<connect gate="-B" pin="IOB1" pad="D21"/>
<connect gate="-B" pin="IOB10" pad="F20"/>
<connect gate="-B" pin="IOB11" pad="G17"/>
<connect gate="-B" pin="IOB12" pad="H16"/>
<connect gate="-B" pin="IOB2" pad="D22"/>
<connect gate="-B" pin="IOB3" pad="G16"/>
<connect gate="-B" pin="IOB4" pad="E22"/>
<connect gate="-B" pin="IOB5" pad="F4"/>
<connect gate="-B" pin="IOB6" pad="E2"/>
<connect gate="-B" pin="IOB7" pad="D1"/>
<connect gate="-B" pin="IOB8" pad="F2"/>
<connect gate="-B" pin="IOB9" pad="F3"/>
<connect gate="-C" pin="IOC1" pad="F21"/>
<connect gate="-C" pin="IOC10" pad="G20"/>
<connect gate="-C" pin="IOC11" pad="H18"/>
<connect gate="-C" pin="IOC12" pad="H19"/>
<connect gate="-C" pin="IOC2" pad="G19"/>
<connect gate="-C" pin="IOC3" pad="H17"/>
<connect gate="-C" pin="IOC4" pad="G6"/>
<connect gate="-C" pin="IOC5" pad="G5"/>
<connect gate="-C" pin="IOC6" pad="F1"/>
<connect gate="-C" pin="IOC7" pad="F22"/>
<connect gate="-C" pin="IOC8" pad="G2"/>
<connect gate="-C" pin="IOC9" pad="G4"/>
<connect gate="-D" pin="IOD10" pad="H6"/>
<connect gate="-D" pin="IOD11" pad="J16"/>
<connect gate="-D" pin="IOD12" pad="J18"/>
<connect gate="-D" pin="IOD3" pad="G22"/>
<connect gate="-D" pin="IOD4" pad="J17"/>
<connect gate="-D" pin="IOD6" pad="H3"/>
<connect gate="-D" pin="IOD7" pad="H1"/>
<connect gate="-D" pin="IOD8" pad="H4"/>
<connect gate="-D" pin="IOD9" pad="H5"/>
<connect gate="-E" pin="IOE1" pad="J19"/>
<connect gate="-E" pin="IOE10" pad="K15"/>
<connect gate="-E" pin="IOE11" pad="K16"/>
<connect gate="-E" pin="IOE2" pad="J2"/>
<connect gate="-E" pin="IOE3" pad="J3"/>
<connect gate="-E" pin="IOE4" pad="J4"/>
<connect gate="-E" pin="IOE5" pad="J7"/>
<connect gate="-E" pin="IOE6" pad="J5"/>
<connect gate="-E" pin="IOE7" pad="H7"/>
<connect gate="-E" pin="IOE8" pad="H21"/>
<connect gate="-E" pin="IOE9" pad="H22"/>
<connect gate="-F" pin="IOF1" pad="J21"/>
<connect gate="-F" pin="IOF10" pad="K17"/>
<connect gate="-F" pin="IOF11" pad="K18"/>
<connect gate="-F" pin="IOF12" pad="K19"/>
<connect gate="-F" pin="IOF2" pad="L15"/>
<connect gate="-F" pin="IOF3" pad="K2"/>
<connect gate="-F" pin="IOF4" pad="K5"/>
<connect gate="-F" pin="IOF5" pad="J6"/>
<connect gate="-F" pin="IOF6" pad="J1"/>
<connect gate="-F" pin="IOF7" pad="J22"/>
<connect gate="-F" pin="IOF8" pad="K1"/>
<connect gate="-F" pin="IOF9" pad="K4"/>
<connect gate="-G" pin="IOG1" pad="L17"/>
<connect gate="-G" pin="IOG10" pad="L18"/>
<connect gate="-G" pin="IOG2" pad="K21"/>
<connect gate="-G" pin="IOG3" pad="K22"/>
<connect gate="-G" pin="IOG4" pad="L5"/>
<connect gate="-G" pin="IOG5" pad="K6"/>
<connect gate="-G" pin="IOG6" pad="K7"/>
<connect gate="-G" pin="IOG7" pad="K8"/>
<connect gate="-G" pin="IOG8" pad="L1"/>
<connect gate="-G" pin="IOG9" pad="L2"/>
<connect gate="-H" pin="IOH1" pad="L22"/>
<connect gate="-H" pin="IOH10" pad="M3"/>
<connect gate="-H" pin="IOH2" pad="L20"/>
<connect gate="-H" pin="IOH3" pad="L19"/>
<connect gate="-H" pin="IOH4" pad="M2"/>
<connect gate="-H" pin="IOH5" pad="L4"/>
<connect gate="-H" pin="IOH6" pad="L3"/>
<connect gate="-H" pin="IOH7" pad="L7"/>
<connect gate="-H" pin="IOH8" pad="L21"/>
<connect gate="-H" pin="IOH9" pad="M1"/>
<connect gate="-I" pin="IOI1" pad="M22"/>
<connect gate="-I" pin="IOI10" pad="N1"/>
<connect gate="-I" pin="IOI2" pad="M21"/>
<connect gate="-I" pin="IOI3" pad="N2"/>
<connect gate="-I" pin="IOI4" pad="L6"/>
<connect gate="-I" pin="IOI5" pad="M4"/>
<connect gate="-I" pin="IOI6" pad="L16"/>
<connect gate="-I" pin="IOI7" pad="M5"/>
<connect gate="-I" pin="IOI8" pad="M6"/>
<connect gate="-I" pin="IOI9" pad="M19"/>
<connect gate="-J" pin="IOJ1" pad="M18"/>
<connect gate="-J" pin="IOJ10" pad="P2"/>
<connect gate="-J" pin="IOJ2" pad="P22"/>
<connect gate="-J" pin="IOJ3" pad="L8"/>
<connect gate="-J" pin="IOJ4" pad="M7"/>
<connect gate="-J" pin="IOJ5" pad="M17"/>
<connect gate="-J" pin="IOJ6" pad="N4"/>
<connect gate="-J" pin="IOJ7" pad="N21"/>
<connect gate="-J" pin="IOJ8" pad="N22"/>
<connect gate="-J" pin="IOJ9" pad="P1"/>
<connect gate="-K" pin="IOK1" pad="M16"/>
<connect gate="-K" pin="IOK10" pad="P21"/>
<connect gate="-K" pin="IOK11" pad="R2"/>
<connect gate="-K" pin="IOK2" pad="P20"/>
<connect gate="-K" pin="IOK3" pad="P3"/>
<connect gate="-K" pin="IOK4" pad="N5"/>
<connect gate="-K" pin="IOK5" pad="M8"/>
<connect gate="-K" pin="IOK6" pad="M15"/>
<connect gate="-K" pin="IOK7" pad="N6"/>
<connect gate="-K" pin="IOK8" pad="N19"/>
<connect gate="-K" pin="IOK9" pad="P4"/>
<connect gate="-L" pin="IOL1" pad="R20"/>
<connect gate="-L" pin="IOL10" pad="R21"/>
<connect gate="-L" pin="IOL2" pad="R3"/>
<connect gate="-L" pin="IOL3" pad="P5"/>
<connect gate="-L" pin="IOL4" pad="N7"/>
<connect gate="-L" pin="IOL5" pad="N8"/>
<connect gate="-L" pin="IOL6" pad="N15"/>
<connect gate="-L" pin="IOL7" pad="N18"/>
<connect gate="-L" pin="IOL8" pad="P19"/>
<connect gate="-L" pin="IOL9" pad="R4"/>
<connect gate="-M" pin="IOM1" pad="N17"/>
<connect gate="-M" pin="IOM10" pad="T21"/>
<connect gate="-M" pin="IOM11" pad="U1"/>
<connect gate="-M" pin="IOM12" pad="U22"/>
<connect gate="-M" pin="IOM2" pad="N16"/>
<connect gate="-M" pin="IOM3" pad="P6"/>
<connect gate="-M" pin="IOM5" pad="P16"/>
<connect gate="-M" pin="IOM6" pad="R5"/>
<connect gate="-M" pin="IOM7" pad="R19"/>
<connect gate="-M" pin="IOM8" pad="T2"/>
<connect gate="-M" pin="IOM9" pad="T4"/>
<connect gate="-N" pin="ION1" pad="P18"/>
<connect gate="-N" pin="ION10" pad="T20"/>
<connect gate="-N" pin="ION11" pad="V1"/>
<connect gate="-N" pin="ION2" pad="U21"/>
<connect gate="-N" pin="ION3" pad="P7"/>
<connect gate="-N" pin="ION4" pad="U2"/>
<connect gate="-N" pin="ION5" pad="P17"/>
<connect gate="-N" pin="ION6" pad="R6"/>
<connect gate="-N" pin="ION7" pad="R7"/>
<connect gate="-N" pin="ION8" pad="R18"/>
<connect gate="-N" pin="ION9" pad="T19"/>
<connect gate="-O" pin="IOO1" pad="U19"/>
<connect gate="-O" pin="IOO10" pad="V2"/>
<connect gate="-O" pin="IOO11" pad="V21"/>
<connect gate="-O" pin="IOO12" pad="W22"/>
<connect gate="-O" pin="IOO2" pad="V20"/>
<connect gate="-O" pin="IOO3" pad="T6"/>
<connect gate="-O" pin="IOO4" pad="T5"/>
<connect gate="-O" pin="IOO5" pad="R17"/>
<connect gate="-O" pin="IOO6" pad="T18"/>
<connect gate="-O" pin="IOO7" pad="U3"/>
<connect gate="-O" pin="IOO8" pad="U5"/>
<connect gate="-O" pin="IOO9" pad="U20"/>
<connect gate="-P" pin="IOP10" pad="T17"/>
<connect gate="-P" pin="IOP11" pad="U6"/>
<connect gate="-P" pin="IOP12" pad="W1"/>
<connect gate="-P" pin="IOP2" pad="V18"/>
<connect gate="-P" pin="IOP3" pad="W3"/>
<connect gate="-P" pin="IOP4" pad="W4"/>
<connect gate="-P" pin="IOP5" pad="W2"/>
<connect gate="-P" pin="IOP6" pad="AA21"/>
<connect gate="-P" pin="IOP7" pad="AB22"/>
<connect gate="-P" pin="IOP8" pad="R16"/>
<connect gate="-P" pin="IOP9" pad="T16"/>
<connect gate="1" pin="VCC" pad="AA12"/>
<connect gate="10" pin="VCC" pad="L10"/>
<connect gate="100" pin="GND" pad="Y22"/>
<connect gate="101" pin="GND" pad="V3"/>
<connect gate="11" pin="VCC" pad="L13"/>
<connect gate="12" pin="VCC" pad="M10"/>
<connect gate="13" pin="VCC" pad="M13"/>
<connect gate="14" pin="VCC" pad="M14"/>
<connect gate="15" pin="VCC" pad="N12"/>
<connect gate="16" pin="VCC" pad="P8"/>
<connect gate="17" pin="VCC" pad="P10"/>
<connect gate="18" pin="VCC" pad="P12"/>
<connect gate="19" pin="VCC" pad="P15"/>
<connect gate="2" pin="VCC" pad="C11"/>
<connect gate="20" pin="VCC" pad="R14"/>
<connect gate="21" pin="VCC" pad="V5"/>
<connect gate="22" pin="VCC" pad="W21"/>
<connect gate="23" pin="VCC" pad="Y8"/>
<connect gate="24" pin="VCCIO" pad="AB13"/>
<connect gate="25" pin="VCCIO" pad="A6"/>
<connect gate="26" pin="VCCIO" pad="A13"/>
<connect gate="27" pin="VCCIO" pad="B5"/>
<connect gate="28" pin="VCCIO" pad="E1"/>
<connect gate="29" pin="VCCIO" pad="G1"/>
<connect gate="3" pin="VCC" pad="C15"/>
<connect gate="30" pin="VCCIO" pad="G15"/>
<connect gate="31" pin="VCCIO" pad="H9"/>
<connect gate="32" pin="VCCIO" pad="H20"/>
<connect gate="33" pin="VCCIO" pad="J11"/>
<connect gate="34" pin="VCCIO" pad="J13"/>
<connect gate="35" pin="VCCIO" pad="K9"/>
<connect gate="36" pin="VCCIO" pad="K11"/>
<connect gate="37" pin="VCCIO" pad="K14"/>
<connect gate="38" pin="VCCIO" pad="K20"/>
<connect gate="39" pin="VCCIO" pad="L14"/>
<connect gate="4" pin="VCC" pad="H14"/>
<connect gate="40" pin="VCCIO" pad="M9"/>
<connect gate="41" pin="VCCIO" pad="N3"/>
<connect gate="42" pin="VCCIO" pad="N9"/>
<connect gate="43" pin="VCCIO" pad="N11"/>
<connect gate="44" pin="VCCIO" pad="N14"/>
<connect gate="45" pin="VCCIO" pad="N20"/>
<connect gate="46" pin="VCCIO" pad="P13"/>
<connect gate="47" pin="VCCIO" pad="R1"/>
<connect gate="48" pin="VCCIO" pad="R9"/>
<connect gate="49" pin="VCCIO" pad="T3"/>
<connect gate="5" pin="VCC" pad="J8"/>
<connect gate="50" pin="VCCIO" pad="T15"/>
<connect gate="51" pin="VCCIO" pad="T22"/>
<connect gate="52" pin="VCCIO" pad="V22"/>
<connect gate="53" pin="GND" pad="AA1"/>
<connect gate="54" pin="GND" pad="AA6"/>
<connect gate="55" pin="GND" pad="AA22"/>
<connect gate="56" pin="GND" pad="AB11"/>
<connect gate="57" pin="GND" pad="AB16"/>
<connect gate="58" pin="GND" pad="A1"/>
<connect gate="59" pin="GND" pad="A8"/>
<connect gate="6" pin="VCC" pad="J10"/>
<connect gate="60" pin="GND" pad="A22"/>
<connect gate="61" pin="GND" pad="B1"/>
<connect gate="62" pin="GND" pad="B2"/>
<connect gate="63" pin="GND" pad="B17"/>
<connect gate="64" pin="GND" pad="B21"/>
<connect gate="65" pin="GND" pad="B22"/>
<connect gate="66" pin="GND" pad="C2"/>
<connect gate="67" pin="GND" pad="C21"/>
<connect gate="68" pin="GND" pad="E21"/>
<connect gate="69" pin="GND" pad="G3"/>
<connect gate="7" pin="VCC" pad="J12"/>
<connect gate="70" pin="GND" pad="G21"/>
<connect gate="71" pin="GND" pad="H2"/>
<connect gate="72" pin="GND" pad="H8"/>
<connect gate="73" pin="GND" pad="H15"/>
<connect gate="74" pin="GND" pad="J9"/>
<connect gate="75" pin="GND" pad="J14"/>
<connect gate="76" pin="GND" pad="J20"/>
<connect gate="77" pin="GND" pad="K3"/>
<connect gate="78" pin="GND" pad="K10"/>
<connect gate="79" pin="GND" pad="K12"/>
<connect gate="8" pin="VCC" pad="J15"/>
<connect gate="80" pin="GND" pad="K13"/>
<connect gate="81" pin="GND" pad="L11"/>
<connect gate="82" pin="GND" pad="L12"/>
<connect gate="83" pin="GND" pad="M11"/>
<connect gate="84" pin="GND" pad="M12"/>
<connect gate="85" pin="GND" pad="M20"/>
<connect gate="86" pin="GND" pad="N10"/>
<connect gate="87" pin="GND" pad="N13"/>
<connect gate="88" pin="GND" pad="P9"/>
<connect gate="89" pin="GND" pad="P14"/>
<connect gate="9" pin="VCC" pad="L9"/>
<connect gate="90" pin="GND" pad="R8"/>
<connect gate="91" pin="GND" pad="R15"/>
<connect gate="92" pin="GND" pad="R22"/>
<connect gate="93" pin="GND" pad="T1"/>
<connect gate="94" pin="GND" pad="W11"/>
<connect gate="95" pin="GND" pad="W20"/>
<connect gate="96" pin="GND" pad="Y1"/>
<connect gate="97" pin="GND" pad="Y2"/>
<connect gate="98" pin="GND" pad="Y3"/>
<connect gate="99" pin="GND" pad="Y21"/>
<connect gate="_" pin="/CE" pad="E4"/>
<connect gate="_" pin="/CEO" pad="E19"/>
<connect gate="_" pin="/CONFIG" pad="T7"/>
<connect gate="_" pin="/STATUS" pad="W19"/>
<connect gate="_" pin="CONF_DONE" pad="F18"/>
<connect gate="_" pin="DATA0" pad="D4"/>
<connect gate="_" pin="DCLK" pad="E5"/>
<connect gate="_" pin="GCLK0" pad="P11"/>
<connect gate="_" pin="GCLK1" pad="D12"/>
<connect gate="_" pin="IN0" pad="R12"/>
<connect gate="_" pin="IN1" pad="V11"/>
<connect gate="_" pin="IN2" pad="H11"/>
<connect gate="_" pin="IN3" pad="E12"/>
<connect gate="_" pin="MSEL0" pad="U4"/>
<connect gate="_" pin="MSEL1" pad="V4"/>
<connect gate="_" pin="TCK" pad="E18"/>
<connect gate="_" pin="TDI" pad="F5"/>
<connect gate="_" pin="TDO" pad="F19"/>
<connect gate="_" pin="TMS" pad="U18"/>
<connect gate="_" pin="TRST" pad="V19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K130EFC484-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8855"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K100A-BGA600" prefix="IC">
<description>&lt;b&gt;EPF10K100&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100B600C"/>
<gate name="-A" symbol="A16"/>
<gate name="-B" symbol="B16"/>
<gate name="-C" symbol="C16"/>
<gate name="-D" symbol="D16"/>
<gate name="-E" symbol="E16"/>
<gate name="-F" symbol="F16"/>
<gate name="-G" symbol="G16"/>
<gate name="-H" symbol="H16"/>
<gate name="-I" symbol="I16"/>
<gate name="-J" symbol="J16"/>
<gate name="-K" symbol="K16"/>
<gate name="-L" symbol="L16"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="-10" symbol="IO404"/>
<gate name="-11" symbol="IO444"/>
<gate name="-12" symbol="IO484"/>
<gate name="-13" symbol="IO524"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="G50" symbol="GND"/>
<gate name="G51" symbol="GND"/>
<gate name="G52" symbol="GND"/>
<gate name="G53" symbol="GND"/>
<gate name="G54" symbol="GND"/>
<gate name="G55" symbol="GND"/>
<gate name="G56" symbol="GND"/>
<gate name="G57" symbol="GND"/>
<gate name="G58" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC40" symbol="NC"/>
<gate name="NC41" symbol="NC"/>
<gate name="NC42" symbol="NC"/>
<gate name="NC43" symbol="NC"/>
<gate name="NC44" symbol="NC"/>
<gate name="NC45" symbol="NC"/>
<gate name="NC46" symbol="NC"/>
<gate name="NC47" symbol="NC"/>
<gate name="NC48" symbol="NC"/>
<gate name="NC49" symbol="NC"/>
<gate name="NC50" symbol="NC"/>
<gate name="NC51" symbol="NC"/>
<gate name="NC52" symbol="NC"/>
<gate name="NC53" symbol="NC"/>
<gate name="NC54" symbol="NC"/>
<gate name="NC55" symbol="NC"/>
<gate name="NC56" symbol="NC"/>
<gate name="NC57" symbol="NC"/>
<gate name="NC58" symbol="NC"/>
<gate name="NC59" symbol="NC"/>
<gate name="NC60" symbol="NC"/>
<gate name="NC61" symbol="NC"/>
<gate name="NC62" symbol="NC"/>
<gate name="NC63" symbol="NC"/>
<gate name="NC64" symbol="NC"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="V24" symbol="VCCINT"/>
<gate name="V25" symbol="VCCINT"/>
<gate name="V26" symbol="VCCINT"/>
<gate name="V27" symbol="VCCINT"/>
<gate name="V28" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="BGA600">
<connects>
<connect gate="-1" pin="IO11" pad="A6"/>
<connect gate="-1" pin="IO12" pad="AR6"/>
<connect gate="-1" pin="IO13" pad="E7"/>
<connect gate="-1" pin="IO14" pad="AL7"/>
<connect gate="-1" pin="IO21" pad="D7"/>
<connect gate="-1" pin="IO22" pad="C7"/>
<connect gate="-1" pin="IO23" pad="AN7"/>
<connect gate="-1" pin="IO24" pad="AM7"/>
<connect gate="-1" pin="IO31" pad="B7"/>
<connect gate="-1" pin="IO32" pad="A7"/>
<connect gate="-1" pin="IO33" pad="AR7"/>
<connect gate="-1" pin="IO34" pad="AP7"/>
<connect gate="-1" pin="IO41" pad="E8"/>
<connect gate="-1" pin="IO42" pad="D8"/>
<connect gate="-1" pin="IO43" pad="AL8"/>
<connect gate="-1" pin="IO44" pad="AM8"/>
<connect gate="-10" pin="IO371" pad="AN23"/>
<connect gate="-10" pin="IO372" pad="E23"/>
<connect gate="-10" pin="IO373" pad="D23"/>
<connect gate="-10" pin="IO374" pad="AP23"/>
<connect gate="-10" pin="IO381" pad="AL23"/>
<connect gate="-10" pin="IO382" pad="A24"/>
<connect gate="-10" pin="IO383" pad="B24"/>
<connect gate="-10" pin="IO384" pad="AM23"/>
<connect gate="-10" pin="IO391" pad="AN24"/>
<connect gate="-10" pin="IO392" pad="C24"/>
<connect gate="-10" pin="IO393" pad="AR24"/>
<connect gate="-10" pin="IO394" pad="A25"/>
<connect gate="-10" pin="IO401" pad="E24"/>
<connect gate="-10" pin="IO402" pad="B25"/>
<connect gate="-10" pin="IO403" pad="AM24"/>
<connect gate="-10" pin="IO404" pad="AR25"/>
<connect gate="-11" pin="IO411" pad="AL24"/>
<connect gate="-11" pin="IO412" pad="AP25"/>
<connect gate="-11" pin="IO413" pad="C25"/>
<connect gate="-11" pin="IO414" pad="D25"/>
<connect gate="-11" pin="IO421" pad="A26"/>
<connect gate="-11" pin="IO422" pad="E25"/>
<connect gate="-11" pin="IO423" pad="AM25"/>
<connect gate="-11" pin="IO424" pad="AN25"/>
<connect gate="-11" pin="IO431" pad="C26"/>
<connect gate="-11" pin="IO432" pad="AR26"/>
<connect gate="-11" pin="IO433" pad="B26"/>
<connect gate="-11" pin="IO434" pad="AL25"/>
<connect gate="-11" pin="IO441" pad="AN26"/>
<connect gate="-11" pin="IO442" pad="D26"/>
<connect gate="-11" pin="IO443" pad="E26"/>
<connect gate="-11" pin="IO444" pad="AP26"/>
<connect gate="-12" pin="IO451" pad="C27"/>
<connect gate="-12" pin="IO452" pad="AR27"/>
<connect gate="-12" pin="IO453" pad="B27"/>
<connect gate="-12" pin="IO454" pad="AL26"/>
<connect gate="-12" pin="IO461" pad="AN27"/>
<connect gate="-12" pin="IO462" pad="E27"/>
<connect gate="-12" pin="IO463" pad="D27"/>
<connect gate="-12" pin="IO464" pad="AP27"/>
<connect gate="-12" pin="IO471" pad="AL27"/>
<connect gate="-12" pin="IO472" pad="A28"/>
<connect gate="-12" pin="IO473" pad="B28"/>
<connect gate="-12" pin="IO474" pad="AM27"/>
<connect gate="-12" pin="IO481" pad="D28"/>
<connect gate="-12" pin="IO482" pad="AP28"/>
<connect gate="-12" pin="IO483" pad="C28"/>
<connect gate="-12" pin="IO484" pad="AR28"/>
<connect gate="-13" pin="IO491" pad="AM28"/>
<connect gate="-13" pin="IO492" pad="A29"/>
<connect gate="-13" pin="IO493" pad="E28"/>
<connect gate="-13" pin="IO494" pad="AN28"/>
<connect gate="-13" pin="IO501" pad="AL28"/>
<connect gate="-13" pin="IO502" pad="AR29"/>
<connect gate="-13" pin="IO503" pad="B29"/>
<connect gate="-13" pin="IO504" pad="C29"/>
<connect gate="-13" pin="IO511" pad="E29"/>
<connect gate="-13" pin="IO512" pad="AN29"/>
<connect gate="-13" pin="IO513" pad="D29"/>
<connect gate="-13" pin="IO514" pad="AP29"/>
<connect gate="-13" pin="IO521" pad="B30"/>
<connect gate="-13" pin="IO522" pad="AL29"/>
<connect gate="-13" pin="IO523" pad="A30"/>
<connect gate="-13" pin="IO524" pad="AM29"/>
<connect gate="-2" pin="IO51" pad="B8"/>
<connect gate="-2" pin="IO52" pad="A8"/>
<connect gate="-2" pin="IO53" pad="AR8"/>
<connect gate="-2" pin="IO54" pad="AP8"/>
<connect gate="-2" pin="IO61" pad="E9"/>
<connect gate="-2" pin="IO62" pad="D9"/>
<connect gate="-2" pin="IO63" pad="AL9"/>
<connect gate="-2" pin="IO64" pad="AM9"/>
<connect gate="-2" pin="IO71" pad="C9"/>
<connect gate="-2" pin="IO72" pad="B9"/>
<connect gate="-2" pin="IO73" pad="AP9"/>
<connect gate="-2" pin="IO74" pad="AN9"/>
<connect gate="-2" pin="IO81" pad="A9"/>
<connect gate="-2" pin="IO82" pad="E10"/>
<connect gate="-2" pin="IO83" pad="AL10"/>
<connect gate="-2" pin="IO84" pad="AR9"/>
<connect gate="-3" pin="IO101" pad="AR10"/>
<connect gate="-3" pin="IO102" pad="B10"/>
<connect gate="-3" pin="IO103" pad="AP10"/>
<connect gate="-3" pin="IO104" pad="A10"/>
<connect gate="-3" pin="IO111" pad="AM11"/>
<connect gate="-3" pin="IO112" pad="D11"/>
<connect gate="-3" pin="IO113" pad="E11"/>
<connect gate="-3" pin="IO114" pad="AL11"/>
<connect gate="-3" pin="IO121" pad="AN11"/>
<connect gate="-3" pin="IO122" pad="AP11"/>
<connect gate="-3" pin="IO123" pad="B11"/>
<connect gate="-3" pin="IO124" pad="C11"/>
<connect gate="-3" pin="IO91" pad="D10"/>
<connect gate="-3" pin="IO92" pad="AN10"/>
<connect gate="-3" pin="IO93" pad="C10"/>
<connect gate="-3" pin="IO94" pad="AM10"/>
<connect gate="-4" pin="IO131" pad="D12"/>
<connect gate="-4" pin="IO132" pad="AN12"/>
<connect gate="-4" pin="IO133" pad="C12"/>
<connect gate="-4" pin="IO134" pad="AM12"/>
<connect gate="-4" pin="IO141" pad="B12"/>
<connect gate="-4" pin="IO142" pad="AP12"/>
<connect gate="-4" pin="IO143" pad="AR12"/>
<connect gate="-4" pin="IO144" pad="A12"/>
<connect gate="-4" pin="IO151" pad="E13"/>
<connect gate="-4" pin="IO152" pad="AM13"/>
<connect gate="-4" pin="IO153" pad="D13"/>
<connect gate="-4" pin="IO154" pad="AL13"/>
<connect gate="-4" pin="IO161" pad="C13"/>
<connect gate="-4" pin="IO162" pad="AP13"/>
<connect gate="-4" pin="IO163" pad="B13"/>
<connect gate="-4" pin="IO164" pad="AN13"/>
<connect gate="-5" pin="IO171" pad="AL14"/>
<connect gate="-5" pin="IO172" pad="E14"/>
<connect gate="-5" pin="IO173" pad="A13"/>
<connect gate="-5" pin="IO174" pad="AR13"/>
<connect gate="-5" pin="IO181" pad="C14"/>
<connect gate="-5" pin="IO182" pad="AN14"/>
<connect gate="-5" pin="IO183" pad="D14"/>
<connect gate="-5" pin="IO184" pad="AM14"/>
<connect gate="-5" pin="IO191" pad="A14"/>
<connect gate="-5" pin="IO192" pad="AR14"/>
<connect gate="-5" pin="IO193" pad="B14"/>
<connect gate="-5" pin="IO194" pad="AP14"/>
<connect gate="-5" pin="IO201" pad="AM15"/>
<connect gate="-5" pin="IO202" pad="D15"/>
<connect gate="-5" pin="IO203" pad="E15"/>
<connect gate="-5" pin="IO204" pad="AL15"/>
<connect gate="-6" pin="IO211" pad="A15"/>
<connect gate="-6" pin="IO212" pad="AR15"/>
<connect gate="-6" pin="IO213" pad="B15"/>
<connect gate="-6" pin="IO214" pad="AP15"/>
<connect gate="-6" pin="IO221" pad="AL16"/>
<connect gate="-6" pin="IO222" pad="AM16"/>
<connect gate="-6" pin="IO223" pad="D16"/>
<connect gate="-6" pin="IO224" pad="E16"/>
<connect gate="-6" pin="IO231" pad="B16"/>
<connect gate="-6" pin="IO232" pad="AP16"/>
<connect gate="-6" pin="IO233" pad="C16"/>
<connect gate="-6" pin="IO234" pad="AN16"/>
<connect gate="-6" pin="IO241" pad="E17"/>
<connect gate="-6" pin="IO242" pad="AL17"/>
<connect gate="-6" pin="IO243" pad="A16"/>
<connect gate="-6" pin="IO244" pad="AR16"/>
<connect gate="-7" pin="IO251" pad="C17"/>
<connect gate="-7" pin="IO252" pad="AN17"/>
<connect gate="-7" pin="IO253" pad="AM17"/>
<connect gate="-7" pin="IO254" pad="D17"/>
<connect gate="-7" pin="IO261" pad="AR17"/>
<connect gate="-7" pin="IO262" pad="B17"/>
<connect gate="-7" pin="IO263" pad="AP17"/>
<connect gate="-7" pin="IO264" pad="A17"/>
<connect gate="-7" pin="IO271" pad="C19"/>
<connect gate="-7" pin="IO272" pad="AR19"/>
<connect gate="-7" pin="IO273" pad="B19"/>
<connect gate="-7" pin="IO274" pad="AP18"/>
<connect gate="-7" pin="IO281" pad="E19"/>
<connect gate="-7" pin="IO282" pad="AP19"/>
<connect gate="-7" pin="IO283" pad="D19"/>
<connect gate="-7" pin="IO284" pad="AN19"/>
<connect gate="-8" pin="IO291" pad="C20"/>
<connect gate="-8" pin="IO292" pad="AL19"/>
<connect gate="-8" pin="IO293" pad="B20"/>
<connect gate="-8" pin="IO294" pad="AR20"/>
<connect gate="-8" pin="IO301" pad="E20"/>
<connect gate="-8" pin="IO302" pad="AN20"/>
<connect gate="-8" pin="IO303" pad="D20"/>
<connect gate="-8" pin="IO304" pad="AP20"/>
<connect gate="-8" pin="IO311" pad="B21"/>
<connect gate="-8" pin="IO312" pad="AL20"/>
<connect gate="-8" pin="IO313" pad="A21"/>
<connect gate="-8" pin="IO314" pad="AM20"/>
<connect gate="-8" pin="IO321" pad="D21"/>
<connect gate="-8" pin="IO322" pad="C21"/>
<connect gate="-8" pin="IO323" pad="AP21"/>
<connect gate="-8" pin="IO324" pad="AR21"/>
<connect gate="-9" pin="IO331" pad="A22"/>
<connect gate="-9" pin="IO332" pad="E21"/>
<connect gate="-9" pin="IO333" pad="AM21"/>
<connect gate="-9" pin="IO334" pad="AN21"/>
<connect gate="-9" pin="IO341" pad="C22"/>
<connect gate="-9" pin="IO342" pad="B22"/>
<connect gate="-9" pin="IO343" pad="AL21"/>
<connect gate="-9" pin="IO344" pad="AR22"/>
<connect gate="-9" pin="IO351" pad="E22"/>
<connect gate="-9" pin="IO352" pad="D22"/>
<connect gate="-9" pin="IO353" pad="AN22"/>
<connect gate="-9" pin="IO354" pad="AP22"/>
<connect gate="-9" pin="IO361" pad="A23"/>
<connect gate="-9" pin="IO362" pad="B23"/>
<connect gate="-9" pin="IO363" pad="AM22"/>
<connect gate="-9" pin="IO364" pad="AL22"/>
<connect gate="-A" pin="IOA1" pad="AL32"/>
<connect gate="-A" pin="IOA10" pad="AJ31"/>
<connect gate="-A" pin="IOA11" pad="AK32"/>
<connect gate="-A" pin="IOA12" pad="AJ1"/>
<connect gate="-A" pin="IOA13" pad="AG3"/>
<connect gate="-A" pin="IOA14" pad="AG2"/>
<connect gate="-A" pin="IOA15" pad="AL33"/>
<connect gate="-A" pin="IOA16" pad="AL34"/>
<connect gate="-A" pin="IOA2" pad="AM33"/>
<connect gate="-A" pin="IOA3" pad="AM35"/>
<connect gate="-A" pin="IOA4" pad="AM34"/>
<connect gate="-A" pin="IOA5" pad="AG4"/>
<connect gate="-A" pin="IOA6" pad="AH2"/>
<connect gate="-A" pin="IOA7" pad="AH4"/>
<connect gate="-A" pin="IOA8" pad="AH3"/>
<connect gate="-A" pin="IOA9" pad="AH1"/>
<connect gate="-B" pin="IOB1" pad="AL35"/>
<connect gate="-B" pin="IOB10" pad="AK33"/>
<connect gate="-B" pin="IOB11" pad="AJ32"/>
<connect gate="-B" pin="IOB12" pad="AJ33"/>
<connect gate="-B" pin="IOB13" pad="AF2"/>
<connect gate="-B" pin="IOB14" pad="AJ34"/>
<connect gate="-B" pin="IOB15" pad="AE5"/>
<connect gate="-B" pin="IOB16" pad="AK34"/>
<connect gate="-B" pin="IOB2" pad="AH31"/>
<connect gate="-B" pin="IOB3" pad="AJ35"/>
<connect gate="-B" pin="IOB4" pad="AE3"/>
<connect gate="-B" pin="IOB5" pad="AF1"/>
<connect gate="-B" pin="IOB6" pad="AF3"/>
<connect gate="-B" pin="IOB7" pad="AF5"/>
<connect gate="-B" pin="IOB8" pad="AG1"/>
<connect gate="-B" pin="IOB9" pad="AF4"/>
<connect gate="-C" pin="IOC1" pad="AH33"/>
<connect gate="-C" pin="IOC10" pad="AD1"/>
<connect gate="-C" pin="IOC11" pad="AH32"/>
<connect gate="-C" pin="IOC12" pad="AD5"/>
<connect gate="-C" pin="IOC13" pad="AG32"/>
<connect gate="-C" pin="IOC14" pad="AH34"/>
<connect gate="-C" pin="IOC15" pad="AG34"/>
<connect gate="-C" pin="IOC16" pad="AH35"/>
<connect gate="-C" pin="IOC2" pad="AG33"/>
<connect gate="-C" pin="IOC3" pad="AC5"/>
<connect gate="-C" pin="IOC4" pad="AD3"/>
<connect gate="-C" pin="IOC5" pad="AE1"/>
<connect gate="-C" pin="IOC6" pad="AE2"/>
<connect gate="-C" pin="IOC7" pad="AD4"/>
<connect gate="-C" pin="IOC8" pad="AD2"/>
<connect gate="-C" pin="IOC9" pad="AG31"/>
<connect gate="-D" pin="IOD1" pad="AG35"/>
<connect gate="-D" pin="IOD10" pad="AC1"/>
<connect gate="-D" pin="IOD11" pad="AF33"/>
<connect gate="-D" pin="IOD12" pad="AC2"/>
<connect gate="-D" pin="IOD13" pad="AB3"/>
<connect gate="-D" pin="IOD14" pad="AF35"/>
<connect gate="-D" pin="IOD15" pad="AB1"/>
<connect gate="-D" pin="IOD16" pad="AB35"/>
<connect gate="-D" pin="IOD2" pad="AF34"/>
<connect gate="-D" pin="IOD3" pad="AE31"/>
<connect gate="-D" pin="IOD4" pad="AE32"/>
<connect gate="-D" pin="IOD5" pad="AB2"/>
<connect gate="-D" pin="IOD6" pad="AB4"/>
<connect gate="-D" pin="IOD7" pad="AC4"/>
<connect gate="-D" pin="IOD8" pad="AC3"/>
<connect gate="-D" pin="IOD9" pad="AF31"/>
<connect gate="-E" pin="IOE1" pad="AA34"/>
<connect gate="-E" pin="IOE10" pad="AA32"/>
<connect gate="-E" pin="IOE11" pad="AA31"/>
<connect gate="-E" pin="IOE12" pad="Y5"/>
<connect gate="-E" pin="IOE13" pad="Y3"/>
<connect gate="-E" pin="IOE14" pad="AA35"/>
<connect gate="-E" pin="IOE15" pad="Y33"/>
<connect gate="-E" pin="IOE16" pad="Y32"/>
<connect gate="-E" pin="IOE2" pad="Y31"/>
<connect gate="-E" pin="IOE3" pad="Y4"/>
<connect gate="-E" pin="IOE4" pad="AA1"/>
<connect gate="-E" pin="IOE5" pad="AA5"/>
<connect gate="-E" pin="IOE6" pad="Y34"/>
<connect gate="-E" pin="IOE7" pad="AA4"/>
<connect gate="-E" pin="IOE8" pad="AA3"/>
<connect gate="-E" pin="IOE9" pad="AA2"/>
<connect gate="-F" pin="IOF1" pad="W32"/>
<connect gate="-F" pin="IOF10" pad="W34"/>
<connect gate="-F" pin="IOF11" pad="W35"/>
<connect gate="-F" pin="IOF12" pad="V33"/>
<connect gate="-F" pin="IOF13" pad="W5"/>
<connect gate="-F" pin="IOF14" pad="Y1"/>
<connect gate="-F" pin="IOF15" pad="W3"/>
<connect gate="-F" pin="IOF16" pad="W1"/>
<connect gate="-F" pin="IOF2" pad="V31"/>
<connect gate="-F" pin="IOF3" pad="V5"/>
<connect gate="-F" pin="IOF4" pad="W2"/>
<connect gate="-F" pin="IOF5" pad="W4"/>
<connect gate="-F" pin="IOF6" pad="W31"/>
<connect gate="-F" pin="IOF7" pad="Y35"/>
<connect gate="-F" pin="IOF8" pad="V4"/>
<connect gate="-F" pin="IOF9" pad="W33"/>
<connect gate="-G" pin="IOG1" pad="U32"/>
<connect gate="-G" pin="IOG10" pad="V34"/>
<connect gate="-G" pin="IOG11" pad="V35"/>
<connect gate="-G" pin="IOG12" pad="U31"/>
<connect gate="-G" pin="IOG13" pad="T5"/>
<connect gate="-G" pin="IOG14" pad="U33"/>
<connect gate="-G" pin="IOG15" pad="U35"/>
<connect gate="-G" pin="IOG16" pad="T31"/>
<connect gate="-G" pin="IOG2" pad="U34"/>
<connect gate="-G" pin="IOG3" pad="U4"/>
<connect gate="-G" pin="IOG4" pad="V3"/>
<connect gate="-G" pin="IOG5" pad="V2"/>
<connect gate="-G" pin="IOG6" pad="V1"/>
<connect gate="-G" pin="IOG7" pad="U5"/>
<connect gate="-G" pin="IOG8" pad="U1"/>
<connect gate="-G" pin="IOG9" pad="U2"/>
<connect gate="-H" pin="IOH1" pad="T34"/>
<connect gate="-H" pin="IOH10" pad="R3"/>
<connect gate="-H" pin="IOH11" pad="R4"/>
<connect gate="-H" pin="IOH12" pad="T32"/>
<connect gate="-H" pin="IOH13" pad="R31"/>
<connect gate="-H" pin="IOH14" pad="R2"/>
<connect gate="-H" pin="IOH15" pad="R34"/>
<connect gate="-H" pin="IOH16" pad="R33"/>
<connect gate="-H" pin="IOH2" pad="R32"/>
<connect gate="-H" pin="IOH3" pad="R35"/>
<connect gate="-H" pin="IOH4" pad="R5"/>
<connect gate="-H" pin="IOH5" pad="T4"/>
<connect gate="-H" pin="IOH6" pad="T3"/>
<connect gate="-H" pin="IOH7" pad="T1"/>
<connect gate="-H" pin="IOH8" pad="T2"/>
<connect gate="-H" pin="IOH9" pad="T33"/>
<connect gate="-I" pin="IOI1" pad="P32"/>
<connect gate="-I" pin="IOI10" pad="P31"/>
<connect gate="-I" pin="IOI11" pad="P34"/>
<connect gate="-I" pin="IOI12" pad="N33"/>
<connect gate="-I" pin="IOI13" pad="N3"/>
<connect gate="-I" pin="IOI14" pad="P33"/>
<connect gate="-I" pin="IOI15" pad="N31"/>
<connect gate="-I" pin="IOI16" pad="N32"/>
<connect gate="-I" pin="IOI2" pad="P35"/>
<connect gate="-I" pin="IOI3" pad="P1"/>
<connect gate="-I" pin="IOI4" pad="R1"/>
<connect gate="-I" pin="IOI5" pad="P3"/>
<connect gate="-I" pin="IOI6" pad="P4"/>
<connect gate="-I" pin="IOI7" pad="N4"/>
<connect gate="-I" pin="IOI8" pad="P2"/>
<connect gate="-I" pin="IOI9" pad="N5"/>
<connect gate="-J" pin="IOJ1" pad="M31"/>
<connect gate="-J" pin="IOJ10" pad="M34"/>
<connect gate="-J" pin="IOJ11" pad="L2"/>
<connect gate="-J" pin="IOJ12" pad="M3"/>
<connect gate="-J" pin="IOJ13" pad="N35"/>
<connect gate="-J" pin="IOJ14" pad="L1"/>
<connect gate="-J" pin="IOJ15" pad="L34"/>
<connect gate="-J" pin="IOJ16" pad="M33"/>
<connect gate="-J" pin="IOJ2" pad="L35"/>
<connect gate="-J" pin="IOJ3" pad="M4"/>
<connect gate="-J" pin="IOJ4" pad="M5"/>
<connect gate="-J" pin="IOJ5" pad="N2"/>
<connect gate="-J" pin="IOJ6" pad="M1"/>
<connect gate="-J" pin="IOJ7" pad="M32"/>
<connect gate="-J" pin="IOJ8" pad="N1"/>
<connect gate="-J" pin="IOJ9" pad="M35"/>
<connect gate="-K" pin="IOK1" pad="K34"/>
<connect gate="-K" pin="IOK10" pad="L4"/>
<connect gate="-K" pin="IOK11" pad="L33"/>
<connect gate="-K" pin="IOK12" pad="K4"/>
<connect gate="-K" pin="IOK13" pad="L31"/>
<connect gate="-K" pin="IOK14" pad="J1"/>
<connect gate="-K" pin="IOK15" pad="K33"/>
<connect gate="-K" pin="IOK16" pad="J35"/>
<connect gate="-K" pin="IOK2" pad="K31"/>
<connect gate="-K" pin="IOK3" pad="K2"/>
<connect gate="-K" pin="IOK4" pad="L3"/>
<connect gate="-K" pin="IOK5" pad="K1"/>
<connect gate="-K" pin="IOK6" pad="L32"/>
<connect gate="-K" pin="IOK7" pad="K35"/>
<connect gate="-K" pin="IOK8" pad="K3"/>
<connect gate="-K" pin="IOK9" pad="L5"/>
<connect gate="-L" pin="IOL1" pad="J32"/>
<connect gate="-L" pin="IOL10" pad="J34"/>
<connect gate="-L" pin="IOL11" pad="J5"/>
<connect gate="-L" pin="IOL12" pad="J33"/>
<connect gate="-L" pin="IOL13" pad="H4"/>
<connect gate="-L" pin="IOL14" pad="H35"/>
<connect gate="-L" pin="IOL15" pad="J31"/>
<connect gate="-L" pin="IOL16" pad="H33"/>
<connect gate="-L" pin="IOL2" pad="H34"/>
<connect gate="-L" pin="IOL3" pad="H32"/>
<connect gate="-L" pin="IOL4" pad="H2"/>
<connect gate="-L" pin="IOL5" pad="J4"/>
<connect gate="-L" pin="IOL6" pad="K5"/>
<connect gate="-L" pin="IOL7" pad="J2"/>
<connect gate="-L" pin="IOL8" pad="H3"/>
<connect gate="-L" pin="IOL9" pad="J3"/>
<connect gate="G1" pin="GND" pad="AL6"/>
<connect gate="G10" pin="GND" pad="AP2"/>
<connect gate="G11" pin="GND" pad="AP3"/>
<connect gate="G12" pin="GND" pad="AP4"/>
<connect gate="G13" pin="GND" pad="AP5"/>
<connect gate="G14" pin="GND" pad="AP6"/>
<connect gate="G15" pin="GND" pad="AP30"/>
<connect gate="G16" pin="GND" pad="AP31"/>
<connect gate="G17" pin="GND" pad="AP32"/>
<connect gate="G18" pin="GND" pad="AP33"/>
<connect gate="G19" pin="GND" pad="AR1"/>
<connect gate="G2" pin="GND" pad="AL30"/>
<connect gate="G20" pin="GND" pad="AR2"/>
<connect gate="G21" pin="GND" pad="AR3"/>
<connect gate="G22" pin="GND" pad="AR4"/>
<connect gate="G23" pin="GND" pad="AR5"/>
<connect gate="G24" pin="GND" pad="AR30"/>
<connect gate="G25" pin="GND" pad="AR31"/>
<connect gate="G26" pin="GND" pad="AR32"/>
<connect gate="G27" pin="GND" pad="AR33"/>
<connect gate="G28" pin="GND" pad="AR34"/>
<connect gate="G29" pin="GND" pad="AR35"/>
<connect gate="G3" pin="GND" pad="AM6"/>
<connect gate="G30" pin="GND" pad="A1"/>
<connect gate="G31" pin="GND" pad="A2"/>
<connect gate="G32" pin="GND" pad="A3"/>
<connect gate="G33" pin="GND" pad="A4"/>
<connect gate="G34" pin="GND" pad="A5"/>
<connect gate="G35" pin="GND" pad="A18"/>
<connect gate="G36" pin="GND" pad="A31"/>
<connect gate="G37" pin="GND" pad="A32"/>
<connect gate="G38" pin="GND" pad="A33"/>
<connect gate="G39" pin="GND" pad="A34"/>
<connect gate="G4" pin="GND" pad="AM30"/>
<connect gate="G40" pin="GND" pad="A35"/>
<connect gate="G41" pin="GND" pad="B2"/>
<connect gate="G42" pin="GND" pad="B3"/>
<connect gate="G43" pin="GND" pad="B4"/>
<connect gate="G44" pin="GND" pad="B5"/>
<connect gate="G45" pin="GND" pad="B6"/>
<connect gate="G46" pin="GND" pad="B31"/>
<connect gate="G47" pin="GND" pad="B32"/>
<connect gate="G48" pin="GND" pad="B33"/>
<connect gate="G49" pin="GND" pad="B34"/>
<connect gate="G5" pin="GND" pad="AN5"/>
<connect gate="G50" pin="GND" pad="B35"/>
<connect gate="G51" pin="GND" pad="C5"/>
<connect gate="G52" pin="GND" pad="C6"/>
<connect gate="G53" pin="GND" pad="C30"/>
<connect gate="G54" pin="GND" pad="C31"/>
<connect gate="G55" pin="GND" pad="D6"/>
<connect gate="G56" pin="GND" pad="D30"/>
<connect gate="G57" pin="GND" pad="E6"/>
<connect gate="G58" pin="GND" pad="E30"/>
<connect gate="G6" pin="GND" pad="AN6"/>
<connect gate="G7" pin="GND" pad="AN30"/>
<connect gate="G8" pin="GND" pad="AN31"/>
<connect gate="G9" pin="GND" pad="AN35"/>
<connect gate="NC1" pin="NC" pad="AB31"/>
<connect gate="NC10" pin="NC" pad="AD31"/>
<connect gate="NC11" pin="NC" pad="AD32"/>
<connect gate="NC12" pin="NC" pad="AD33"/>
<connect gate="NC13" pin="NC" pad="AD34"/>
<connect gate="NC14" pin="NC" pad="AE33"/>
<connect gate="NC15" pin="NC" pad="AE34"/>
<connect gate="NC16" pin="NC" pad="AE35"/>
<connect gate="NC17" pin="NC" pad="AH5"/>
<connect gate="NC18" pin="NC" pad="AJ2"/>
<connect gate="NC19" pin="NC" pad="AJ3"/>
<connect gate="NC2" pin="NC" pad="AB32"/>
<connect gate="NC20" pin="NC" pad="AJ4"/>
<connect gate="NC21" pin="NC" pad="AJ5"/>
<connect gate="NC22" pin="NC" pad="AK1"/>
<connect gate="NC23" pin="NC" pad="AK2"/>
<connect gate="NC24" pin="NC" pad="AK3"/>
<connect gate="NC25" pin="NC" pad="AK4"/>
<connect gate="NC26" pin="NC" pad="AK5"/>
<connect gate="NC27" pin="NC" pad="AL1"/>
<connect gate="NC28" pin="NC" pad="AL2"/>
<connect gate="NC29" pin="NC" pad="AL4"/>
<connect gate="NC3" pin="NC" pad="AB33"/>
<connect gate="NC30" pin="NC" pad="AM1"/>
<connect gate="NC31" pin="NC" pad="AM2"/>
<connect gate="NC32" pin="NC" pad="AM3"/>
<connect gate="NC33" pin="NC" pad="D1"/>
<connect gate="NC34" pin="NC" pad="D2"/>
<connect gate="NC35" pin="NC" pad="D3"/>
<connect gate="NC36" pin="NC" pad="D33"/>
<connect gate="NC37" pin="NC" pad="D34"/>
<connect gate="NC38" pin="NC" pad="D35"/>
<connect gate="NC39" pin="NC" pad="E1"/>
<connect gate="NC4" pin="NC" pad="AB34"/>
<connect gate="NC40" pin="NC" pad="E3"/>
<connect gate="NC41" pin="NC" pad="E4"/>
<connect gate="NC42" pin="NC" pad="E32"/>
<connect gate="NC43" pin="NC" pad="E33"/>
<connect gate="NC44" pin="NC" pad="E34"/>
<connect gate="NC45" pin="NC" pad="E35"/>
<connect gate="NC46" pin="NC" pad="F1"/>
<connect gate="NC47" pin="NC" pad="F2"/>
<connect gate="NC48" pin="NC" pad="F3"/>
<connect gate="NC49" pin="NC" pad="F4"/>
<connect gate="NC5" pin="NC" pad="AC31"/>
<connect gate="NC50" pin="NC" pad="F32"/>
<connect gate="NC51" pin="NC" pad="F33"/>
<connect gate="NC52" pin="NC" pad="F34"/>
<connect gate="NC53" pin="NC" pad="G1"/>
<connect gate="NC54" pin="NC" pad="G2"/>
<connect gate="NC55" pin="NC" pad="G3"/>
<connect gate="NC56" pin="NC" pad="G4"/>
<connect gate="NC57" pin="NC" pad="G5"/>
<connect gate="NC58" pin="NC" pad="G31"/>
<connect gate="NC59" pin="NC" pad="G32"/>
<connect gate="NC6" pin="NC" pad="AC32"/>
<connect gate="NC60" pin="NC" pad="G33"/>
<connect gate="NC61" pin="NC" pad="G34"/>
<connect gate="NC62" pin="NC" pad="G35"/>
<connect gate="NC63" pin="NC" pad="H5"/>
<connect gate="NC64" pin="NC" pad="H31"/>
<connect gate="NC7" pin="NC" pad="AC33"/>
<connect gate="NC8" pin="NC" pad="AC34"/>
<connect gate="NC9" pin="NC" pad="AC35"/>
<connect gate="V1" pin="VCC" pad="AA33"/>
<connect gate="V10" pin="VCC" pad="AR11"/>
<connect gate="V11" pin="VCC" pad="AR18"/>
<connect gate="V12" pin="VCC" pad="A11"/>
<connect gate="V13" pin="VCC" pad="A19"/>
<connect gate="V14" pin="VCC" pad="B1"/>
<connect gate="V15" pin="VCC" pad="B18"/>
<connect gate="V16" pin="VCC" pad="D24"/>
<connect gate="V17" pin="VCC" pad="E2"/>
<connect gate="V18" pin="VCC" pad="F31"/>
<connect gate="V19" pin="VCC" pad="F35"/>
<connect gate="V2" pin="VCC" pad="AB5"/>
<connect gate="V20" pin="VCC" pad="H1"/>
<connect gate="V21" pin="VCC" pad="K32"/>
<connect gate="V22" pin="VCC" pad="M2"/>
<connect gate="V23" pin="VCC" pad="N34"/>
<connect gate="V24" pin="VCC" pad="P5"/>
<connect gate="V25" pin="VCC" pad="T35"/>
<connect gate="V26" pin="VCC" pad="U3"/>
<connect gate="V27" pin="VCC" pad="V32"/>
<connect gate="V28" pin="VCC" pad="Y2"/>
<connect gate="V3" pin="VCC" pad="AD35"/>
<connect gate="V4" pin="VCC" pad="AE4"/>
<connect gate="V5" pin="VCC" pad="AF32"/>
<connect gate="V6" pin="VCC" pad="AG5"/>
<connect gate="V7" pin="VCC" pad="AK31"/>
<connect gate="V8" pin="VCC" pad="AK35"/>
<connect gate="V9" pin="VCC" pad="AL3"/>
<connect gate="VO1" pin="VCCIO" pad="AL5"/>
<connect gate="VO10" pin="VCCIO" pad="AN15"/>
<connect gate="VO11" pin="VCCIO" pad="AN32"/>
<connect gate="VO12" pin="VCCIO" pad="AN33"/>
<connect gate="VO13" pin="VCCIO" pad="AP34"/>
<connect gate="VO14" pin="VCCIO" pad="AR23"/>
<connect gate="VO15" pin="VCCIO" pad="A20"/>
<connect gate="VO16" pin="VCCIO" pad="A27"/>
<connect gate="VO17" pin="VCCIO" pad="C2"/>
<connect gate="VO18" pin="VCCIO" pad="C3"/>
<connect gate="VO19" pin="VCCIO" pad="C4"/>
<connect gate="VO2" pin="VCCIO" pad="AL12"/>
<connect gate="VO20" pin="VCCIO" pad="C8"/>
<connect gate="VO21" pin="VCCIO" pad="C15"/>
<connect gate="VO22" pin="VCCIO" pad="C23"/>
<connect gate="VO23" pin="VCCIO" pad="C32"/>
<connect gate="VO24" pin="VCCIO" pad="C33"/>
<connect gate="VO25" pin="VCCIO" pad="D5"/>
<connect gate="VO26" pin="VCCIO" pad="D31"/>
<connect gate="VO27" pin="VCCIO" pad="E5"/>
<connect gate="VO28" pin="VCCIO" pad="E12"/>
<connect gate="VO29" pin="VCCIO" pad="E31"/>
<connect gate="VO3" pin="VCCIO" pad="AM5"/>
<connect gate="VO4" pin="VCCIO" pad="AM19"/>
<connect gate="VO5" pin="VCCIO" pad="AM26"/>
<connect gate="VO6" pin="VCCIO" pad="AM31"/>
<connect gate="VO7" pin="VCCIO" pad="AN3"/>
<connect gate="VO8" pin="VCCIO" pad="AN4"/>
<connect gate="VO9" pin="VCCIO" pad="AN8"/>
<connect gate="_" pin="/CE" pad="AN2"/>
<connect gate="_" pin="/CEO" pad="AP35"/>
<connect gate="_" pin="/CONFIG" pad="D4"/>
<connect gate="_" pin="/STATUS" pad="D32"/>
<connect gate="_" pin="CONF_DONE" pad="AM32"/>
<connect gate="_" pin="DATA0" pad="AM4"/>
<connect gate="_" pin="DCLK" pad="AP1"/>
<connect gate="_" pin="GCLK" pad="AL18"/>
<connect gate="_" pin="GCLK1" pad="E18"/>
<connect gate="_" pin="IN0" pad="D18"/>
<connect gate="_" pin="IN1" pad="C18"/>
<connect gate="_" pin="IN2" pad="AN18"/>
<connect gate="_" pin="IN3" pad="AM18"/>
<connect gate="_" pin="MSEL0" pad="F5"/>
<connect gate="_" pin="MSEL1" pad="C1"/>
<connect gate="_" pin="TCK" pad="AL31"/>
<connect gate="_" pin="TDI" pad="AN1"/>
<connect gate="_" pin="TDO" pad="AN34"/>
<connect gate="_" pin="TMS" pad="C35"/>
<connect gate="_" pin="TRST" pad="C34"/>
<connect gate="_" pin="VCC_CKLK" pad="AP24"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K100ABC600-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8783"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K100-PGA503" prefix="IC">
<description>&lt;b&gt;EPF10K100&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100P503C"/>
<gate name="-A" symbol="A16"/>
<gate name="-B" symbol="B16"/>
<gate name="-C" symbol="C16"/>
<gate name="-D" symbol="D16"/>
<gate name="-E" symbol="E16"/>
<gate name="-F" symbol="F16"/>
<gate name="-G" symbol="G16"/>
<gate name="-H" symbol="H16"/>
<gate name="-I" symbol="I16"/>
<gate name="-J" symbol="J16"/>
<gate name="-K" symbol="K16"/>
<gate name="-L" symbol="L16"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="-10" symbol="IO404"/>
<gate name="-11" symbol="IO444"/>
<gate name="-12" symbol="IO484"/>
<gate name="-13" symbol="IO524"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCINT"/>
<gate name="14" symbol="VCCINT"/>
<gate name="15" symbol="VCCINT"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="19" symbol="VCCIO"/>
<gate name="20" symbol="VCCIO"/>
<gate name="21" symbol="VCCIO"/>
<gate name="22" symbol="VCCIO"/>
<gate name="23" symbol="VCCIO"/>
<gate name="24" symbol="VCCIO"/>
<gate name="25" symbol="VCCIO"/>
<gate name="26" symbol="VCCIO"/>
<gate name="27" symbol="VCCIO"/>
<gate name="28" symbol="VCCIO"/>
<gate name="29" symbol="VCCIO"/>
<gate name="30" symbol="VCCIO"/>
<gate name="31" symbol="VCCIO"/>
<gate name="32" symbol="VCCIO"/>
<gate name="33" symbol="VCCIO"/>
<gate name="34" symbol="VCCIO"/>
<gate name="35" symbol="VCCIO"/>
<gate name="36" symbol="VCCIO"/>
<gate name="37" symbol="VCCIO"/>
<gate name="38" symbol="VCCIO"/>
<gate name="39" symbol="VCCIO"/>
<gate name="40" symbol="VCCIO"/>
<gate name="41" symbol="GNDINT"/>
<gate name="42" symbol="GNDINT"/>
<gate name="43" symbol="GNDINT"/>
<gate name="44" symbol="GNDINT"/>
<gate name="45" symbol="GNDINT"/>
<gate name="46" symbol="GNDINT"/>
<gate name="47" symbol="GNDINT"/>
<gate name="48" symbol="GNDINT"/>
<gate name="49" symbol="GNDINT"/>
<gate name="50" symbol="GNDINT"/>
<gate name="51" symbol="GNDINT"/>
<gate name="52" symbol="GNDINT"/>
<gate name="53" symbol="GNDINT"/>
<gate name="54" symbol="GNDINT"/>
<gate name="55" symbol="GNDINT"/>
<gate name="56" symbol="GNDINT"/>
<gate name="58" symbol="GNDIO"/>
<gate name="59" symbol="GNDIO"/>
<gate name="60" symbol="GNDIO"/>
<gate name="61" symbol="GNDIO"/>
<gate name="62" symbol="GNDIO"/>
<gate name="63" symbol="GNDIO"/>
<gate name="64" symbol="GNDIO"/>
<gate name="65" symbol="GNDIO"/>
<gate name="66" symbol="GNDIO"/>
<gate name="67" symbol="GNDIO"/>
<gate name="68" symbol="GNDIO"/>
<gate name="69" symbol="GNDIO"/>
<gate name="70" symbol="GNDIO"/>
<gate name="71" symbol="GNDIO"/>
<gate name="72" symbol="GNDIO"/>
<gate name="73" symbol="GNDIO"/>
<gate name="74" symbol="GNDIO"/>
<gate name="75" symbol="GNDIO"/>
<gate name="76" symbol="GNDIO"/>
<gate name="77" symbol="GNDIO"/>
<gate name="78" symbol="GNDIO"/>
<gate name="79" symbol="GNDIO"/>
<gate name="80" symbol="GNDIO"/>
<gate name="81" symbol="GNDIO"/>
<gate name="82" symbol="GNDIO"/>
</gates>
<devices>
<device name="" package="PGA503">
<connects>
<connect gate="-1" pin="IO11" pad="AY42"/>
<connect gate="-1" pin="IO12" pad="A41"/>
<connect gate="-1" pin="IO13" pad="BA43"/>
<connect gate="-1" pin="IO14" pad="F36"/>
<connect gate="-1" pin="IO21" pad="AV38"/>
<connect gate="-1" pin="IO22" pad="BA41"/>
<connect gate="-1" pin="IO23" pad="B38"/>
<connect gate="-1" pin="IO24" pad="B40"/>
<connect gate="-1" pin="IO31" pad="BB42"/>
<connect gate="-1" pin="IO32" pad="BC43"/>
<connect gate="-1" pin="IO33" pad="D36"/>
<connect gate="-1" pin="IO34" pad="D38"/>
<connect gate="-1" pin="IO41" pad="BC41"/>
<connect gate="-1" pin="IO42" pad="BB40"/>
<connect gate="-1" pin="IO43" pad="E37"/>
<connect gate="-1" pin="IO44" pad="F34"/>
<connect gate="-10" pin="IO371" pad="C13"/>
<connect gate="-10" pin="IO372" pad="BA15"/>
<connect gate="-10" pin="IO373" pad="BC15"/>
<connect gate="-10" pin="IO374" pad="G15"/>
<connect gate="-10" pin="IO381" pad="F14"/>
<connect gate="-10" pin="IO382" pad="AV16"/>
<connect gate="-10" pin="IO383" pad="BB14"/>
<connect gate="-10" pin="IO384" pad="B12"/>
<connect gate="-10" pin="IO391" pad="D12"/>
<connect gate="-10" pin="IO392" pad="AW15"/>
<connect gate="-10" pin="IO393" pad="A11"/>
<connect gate="-10" pin="IO394" pad="BC13"/>
<connect gate="-10" pin="IO401" pad="AU15"/>
<connect gate="-10" pin="IO402" pad="AY14"/>
<connect gate="-10" pin="IO403" pad="B10"/>
<connect gate="-10" pin="IO404" pad="G13"/>
<connect gate="-11" pin="IO411" pad="F12"/>
<connect gate="-11" pin="IO412" pad="A9"/>
<connect gate="-11" pin="IO413" pad="BB12"/>
<connect gate="-11" pin="IO414" pad="BC11"/>
<connect gate="-11" pin="IO421" pad="AU13"/>
<connect gate="-11" pin="IO422" pad="AY12"/>
<connect gate="-11" pin="IO423" pad="D10"/>
<connect gate="-11" pin="IO424" pad="E11"/>
<connect gate="-11" pin="IO431" pad="BC9"/>
<connect gate="-11" pin="IO432" pad="A7"/>
<connect gate="-11" pin="IO433" pad="BB10"/>
<connect gate="-11" pin="IO434" pad="B8"/>
<connect gate="-11" pin="IO441" pad="F10"/>
<connect gate="-11" pin="IO442" pad="AV12"/>
<connect gate="-11" pin="IO443" pad="AW11"/>
<connect gate="-11" pin="IO444" pad="G11"/>
<connect gate="-12" pin="IO451" pad="BB8"/>
<connect gate="-12" pin="IO452" pad="D8"/>
<connect gate="-12" pin="IO453" pad="AY10"/>
<connect gate="-12" pin="IO454" pad="E9"/>
<connect gate="-12" pin="IO461" pad="B6"/>
<connect gate="-12" pin="IO462" pad="AU11"/>
<connect gate="-12" pin="IO463" pad="BC7"/>
<connect gate="-12" pin="IO464" pad="C7"/>
<connect gate="-12" pin="IO471" pad="F8"/>
<connect gate="-12" pin="IO472" pad="AV10"/>
<connect gate="-12" pin="IO473" pad="AW9"/>
<connect gate="-12" pin="IO474" pad="A5"/>
<connect gate="-12" pin="IO481" pad="BB6"/>
<connect gate="-12" pin="IO482" pad="D6"/>
<connect gate="-12" pin="IO483" pad="AY8"/>
<connect gate="-12" pin="IO484" pad="G9"/>
<connect gate="-13" pin="IO491" pad="C5"/>
<connect gate="-13" pin="IO492" pad="AU9"/>
<connect gate="-13" pin="IO493" pad="BC5"/>
<connect gate="-13" pin="IO494" pad="E7"/>
<connect gate="-13" pin="IO501" pad="B4"/>
<connect gate="-13" pin="IO502" pad="A3"/>
<connect gate="-13" pin="IO503" pad="AV8"/>
<connect gate="-13" pin="IO504" pad="AW7"/>
<connect gate="-13" pin="IO511" pad="BA5"/>
<connect gate="-13" pin="IO512" pad="C3"/>
<connect gate="-13" pin="IO513" pad="AY6"/>
<connect gate="-13" pin="IO514" pad="B2"/>
<connect gate="-13" pin="IO521" pad="BC3"/>
<connect gate="-13" pin="IO522" pad="C1"/>
<connect gate="-13" pin="IO523" pad="BB4"/>
<connect gate="-13" pin="IO524" pad="F6"/>
<connect gate="-2" pin="IO51" pad="BA39"/>
<connect gate="-2" pin="IO52" pad="AY38"/>
<connect gate="-2" pin="IO53" pad="B36"/>
<connect gate="-2" pin="IO54" pad="G35"/>
<connect gate="-2" pin="IO61" pad="AW37"/>
<connect gate="-2" pin="IO62" pad="AV36"/>
<connect gate="-2" pin="IO63" pad="A39"/>
<connect gate="-2" pin="IO64" pad="D34"/>
<connect gate="-2" pin="IO71" pad="AU35"/>
<connect gate="-2" pin="IO72" pad="BC39"/>
<connect gate="-2" pin="IO73" pad="E35"/>
<connect gate="-2" pin="IO74" pad="F32"/>
<connect gate="-2" pin="IO81" pad="BB38"/>
<connect gate="-2" pin="IO82" pad="AY36"/>
<connect gate="-2" pin="IO83" pad="A37"/>
<connect gate="-2" pin="IO84" pad="G33"/>
<connect gate="-3" pin="IO101" pad="B34"/>
<connect gate="-3" pin="IO102" pad="AU33"/>
<connect gate="-3" pin="IO103" pad="A35"/>
<connect gate="-3" pin="IO104" pad="BC37"/>
<connect gate="-3" pin="IO111" pad="D32"/>
<connect gate="-3" pin="IO112" pad="BA35"/>
<connect gate="-3" pin="IO113" pad="BB36"/>
<connect gate="-3" pin="IO114" pad="G31"/>
<connect gate="-3" pin="IO121" pad="A33"/>
<connect gate="-3" pin="IO122" pad="B32"/>
<connect gate="-3" pin="IO123" pad="AW33"/>
<connect gate="-3" pin="IO124" pad="AY34"/>
<connect gate="-3" pin="IO91" pad="AW35"/>
<connect gate="-3" pin="IO92" pad="E33"/>
<connect gate="-3" pin="IO93" pad="AV34"/>
<connect gate="-3" pin="IO94" pad="C35"/>
<connect gate="-4" pin="IO131" pad="AV32"/>
<connect gate="-4" pin="IO132" pad="C31"/>
<connect gate="-4" pin="IO133" pad="BC35"/>
<connect gate="-4" pin="IO134" pad="F30"/>
<connect gate="-4" pin="IO141" pad="AU31"/>
<connect gate="-4" pin="IO142" pad="G29"/>
<connect gate="-4" pin="IO143" pad="D30"/>
<connect gate="-4" pin="IO144" pad="BB34"/>
<connect gate="-4" pin="IO151" pad="BA33"/>
<connect gate="-4" pin="IO152" pad="E29"/>
<connect gate="-4" pin="IO153" pad="AY32"/>
<connect gate="-4" pin="IO154" pad="A31"/>
<connect gate="-4" pin="IO161" pad="BC33"/>
<connect gate="-4" pin="IO162" pad="F28"/>
<connect gate="-4" pin="IO163" pad="AV30"/>
<connect gate="-4" pin="IO164" pad="B30"/>
<connect gate="-5" pin="IO171" pad="A29"/>
<connect gate="-5" pin="IO172" pad="BA31"/>
<connect gate="-5" pin="IO173" pad="BB32"/>
<connect gate="-5" pin="IO174" pad="C29"/>
<connect gate="-5" pin="IO181" pad="AY30"/>
<connect gate="-5" pin="IO182" pad="B28"/>
<connect gate="-5" pin="IO183" pad="AU29"/>
<connect gate="-5" pin="IO184" pad="D28"/>
<connect gate="-5" pin="IO191" pad="AW29"/>
<connect gate="-5" pin="IO192" pad="C27"/>
<connect gate="-5" pin="IO193" pad="BC31"/>
<connect gate="-5" pin="IO194" pad="E27"/>
<connect gate="-5" pin="IO201" pad="A27"/>
<connect gate="-5" pin="IO202" pad="AV28"/>
<connect gate="-5" pin="IO203" pad="BB30"/>
<connect gate="-5" pin="IO204" pad="F26"/>
<connect gate="-6" pin="IO211" pad="BC29"/>
<connect gate="-6" pin="IO212" pad="B26"/>
<connect gate="-6" pin="IO213" pad="AY28"/>
<connect gate="-6" pin="IO214" pad="D26"/>
<connect gate="-6" pin="IO221" pad="G25"/>
<connect gate="-6" pin="IO222" pad="A25"/>
<connect gate="-6" pin="IO223" pad="AW27"/>
<connect gate="-6" pin="IO224" pad="BB28"/>
<connect gate="-6" pin="IO231" pad="BC27"/>
<connect gate="-6" pin="IO232" pad="F24"/>
<connect gate="-6" pin="IO233" pad="AV26"/>
<connect gate="-6" pin="IO234" pad="B24"/>
<connect gate="-6" pin="IO241" pad="AU25"/>
<connect gate="-6" pin="IO242" pad="E23"/>
<connect gate="-6" pin="IO243" pad="AY26"/>
<connect gate="-6" pin="IO244" pad="G23"/>
<connect gate="-7" pin="IO251" pad="BC25"/>
<connect gate="-7" pin="IO252" pad="B22"/>
<connect gate="-7" pin="IO253" pad="A23"/>
<connect gate="-7" pin="IO254" pad="BB26"/>
<connect gate="-7" pin="IO261" pad="F22"/>
<connect gate="-7" pin="IO262" pad="AV24"/>
<connect gate="-7" pin="IO263" pad="A21"/>
<connect gate="-7" pin="IO264" pad="BB24"/>
<connect gate="-7" pin="IO271" pad="AW23"/>
<connect gate="-7" pin="IO272" pad="G21"/>
<connect gate="-7" pin="IO273" pad="AU23"/>
<connect gate="-7" pin="IO274" pad="E21"/>
<connect gate="-7" pin="IO281" pad="AV22"/>
<connect gate="-7" pin="IO282" pad="B20"/>
<connect gate="-7" pin="IO283" pad="BC23"/>
<connect gate="-7" pin="IO284" pad="F20"/>
<connect gate="-8" pin="IO291" pad="BC21"/>
<connect gate="-8" pin="IO292" pad="A19"/>
<connect gate="-8" pin="IO293" pad="BB22"/>
<connect gate="-8" pin="IO294" pad="C19"/>
<connect gate="-8" pin="IO301" pad="AU21"/>
<connect gate="-8" pin="IO302" pad="G19"/>
<connect gate="-8" pin="IO303" pad="AW21"/>
<connect gate="-8" pin="IO304" pad="B18"/>
<connect gate="-8" pin="IO311" pad="AV20"/>
<connect gate="-8" pin="IO312" pad="A17"/>
<connect gate="-8" pin="IO313" pad="BB20"/>
<connect gate="-8" pin="IO314" pad="D18"/>
<connect gate="-8" pin="IO321" pad="AU19"/>
<connect gate="-8" pin="IO322" pad="BC19"/>
<connect gate="-8" pin="IO323" pad="E17"/>
<connect gate="-8" pin="IO324" pad="F18"/>
<connect gate="-9" pin="IO331" pad="AY18"/>
<connect gate="-9" pin="IO332" pad="BB18"/>
<connect gate="-9" pin="IO333" pad="A15"/>
<connect gate="-9" pin="IO334" pad="B16"/>
<connect gate="-9" pin="IO341" pad="AV18"/>
<connect gate="-9" pin="IO342" pad="BC17"/>
<connect gate="-9" pin="IO343" pad="D16"/>
<connect gate="-9" pin="IO344" pad="F16"/>
<connect gate="-9" pin="IO351" pad="BB16"/>
<connect gate="-9" pin="IO352" pad="AW17"/>
<connect gate="-9" pin="IO353" pad="E15"/>
<connect gate="-9" pin="IO354" pad="B14"/>
<connect gate="-9" pin="IO361" pad="AV14"/>
<connect gate="-9" pin="IO362" pad="AY16"/>
<connect gate="-9" pin="IO363" pad="A13"/>
<connect gate="-9" pin="IO364" pad="D14"/>
<connect gate="-A" pin="IOA1" pad="D2"/>
<connect gate="-A" pin="IOA10" pad="E1"/>
<connect gate="-A" pin="IOA11" pad="F2"/>
<connect gate="-A" pin="IOA12" pad="F38"/>
<connect gate="-A" pin="IOA13" pad="G39"/>
<connect gate="-A" pin="IOA14" pad="H38"/>
<connect gate="-A" pin="IOA15" pad="J5"/>
<connect gate="-A" pin="IOA16" pad="K6"/>
<connect gate="-A" pin="IOA2" pad="G5"/>
<connect gate="-A" pin="IOA3" pad="J7"/>
<connect gate="-A" pin="IOA4" pad="H6"/>
<connect gate="-A" pin="IOA5" pad="D42"/>
<connect gate="-A" pin="IOA6" pad="A43"/>
<connect gate="-A" pin="IOA7" pad="D40"/>
<connect gate="-A" pin="IOA8" pad="B42"/>
<connect gate="-A" pin="IOA9" pad="C43"/>
<connect gate="-B" pin="IOB1" pad="L7"/>
<connect gate="-B" pin="IOB10" pad="G1"/>
<connect gate="-B" pin="IOB11" pad="H2"/>
<connect gate="-B" pin="IOB12" pad="J1"/>
<connect gate="-B" pin="IOB13" pad="J39"/>
<connect gate="-B" pin="IOB14" pad="K2"/>
<connect gate="-B" pin="IOB15" pad="L37"/>
<connect gate="-B" pin="IOB16" pad="M6"/>
<connect gate="-B" pin="IOB2" pad="L5"/>
<connect gate="-B" pin="IOB3" pad="N7"/>
<connect gate="-B" pin="IOB4" pad="G43"/>
<connect gate="-B" pin="IOB5" pad="K38"/>
<connect gate="-B" pin="IOB6" pad="G41"/>
<connect gate="-B" pin="IOB7" pad="J37"/>
<connect gate="-B" pin="IOB8" pad="E43"/>
<connect gate="-B" pin="IOB9" pad="F42"/>
<connect gate="-C" pin="IOC1" pad="M2"/>
<connect gate="-C" pin="IOC10" pad="L41"/>
<connect gate="-C" pin="IOC11" pad="M4"/>
<connect gate="-C" pin="IOC12" pad="M38"/>
<connect gate="-C" pin="IOC13" pad="P4"/>
<connect gate="-C" pin="IOC14" pad="P6"/>
<connect gate="-C" pin="IOC15" pad="R5"/>
<connect gate="-C" pin="IOC16" pad="R7"/>
<connect gate="-C" pin="IOC2" pad="N1"/>
<connect gate="-C" pin="IOC3" pad="L43"/>
<connect gate="-C" pin="IOC4" pad="N37"/>
<connect gate="-C" pin="IOC5" pad="L39"/>
<connect gate="-C" pin="IOC6" pad="H42"/>
<connect gate="-C" pin="IOC7" pad="J43"/>
<connect gate="-C" pin="IOC8" pad="K42"/>
<connect gate="-C" pin="IOC9" pad="L1"/>
<connect gate="-D" pin="IOD1" pad="T6"/>
<connect gate="-D" pin="IOD10" pad="P40"/>
<connect gate="-D" pin="IOD11" pad="R1"/>
<connect gate="-D" pin="IOD12" pad="R37"/>
<connect gate="-D" pin="IOD13" pad="R39"/>
<connect gate="-D" pin="IOD14" pad="T2"/>
<connect gate="-D" pin="IOD15" pad="T38"/>
<connect gate="-D" pin="IOD16" pad="U1"/>
<connect gate="-D" pin="IOD2" pad="T4"/>
<connect gate="-D" pin="IOD3" pad="U5"/>
<connect gate="-D" pin="IOD4" pad="V6"/>
<connect gate="-D" pin="IOD5" pad="P42"/>
<connect gate="-D" pin="IOD6" pad="N43"/>
<connect gate="-D" pin="IOD7" pad="P38"/>
<connect gate="-D" pin="IOD8" pad="M42"/>
<connect gate="-D" pin="IOD9" pad="P2"/>
<connect gate="-E" pin="IOE1" pad="W7"/>
<connect gate="-E" pin="IOE10" pad="V2"/>
<connect gate="-E" pin="IOE11" pad="V4"/>
<connect gate="-E" pin="IOE12" pad="V38"/>
<connect gate="-E" pin="IOE13" pad="V40"/>
<connect gate="-E" pin="IOE14" pad="W1"/>
<connect gate="-E" pin="IOE15" pad="Y2"/>
<connect gate="-E" pin="IOE16" pad="Y4"/>
<connect gate="-E" pin="IOE2" pad="Y6"/>
<connect gate="-E" pin="IOE3" pad="U43"/>
<connect gate="-E" pin="IOE4" pad="U41"/>
<connect gate="-E" pin="IOE5" pad="T40"/>
<connect gate="-E" pin="IOE6" pad="AA7"/>
<connect gate="-E" pin="IOE7" pad="R43"/>
<connect gate="-E" pin="IOE8" pad="T42"/>
<connect gate="-E" pin="IOE9" pad="U39"/>
<connect gate="-F" pin="IOF1" pad="AB2"/>
<connect gate="-F" pin="IOF10" pad="AB6"/>
<connect gate="-F" pin="IOF11" pad="AC1"/>
<connect gate="-F" pin="IOF12" pad="AC7"/>
<connect gate="-F" pin="IOF13" pad="V42"/>
<connect gate="-F" pin="IOF14" pad="W37"/>
<connect gate="-F" pin="IOF15" pad="Y38"/>
<connect gate="-F" pin="IOF16" pad="Y42"/>
<connect gate="-F" pin="IOF2" pad="AC5"/>
<connect gate="-F" pin="IOF3" pad="AA37"/>
<connect gate="-F" pin="IOF4" pad="Y40"/>
<connect gate="-F" pin="IOF5" pad="W43"/>
<connect gate="-F" pin="IOF6" pad="AA1"/>
<connect gate="-F" pin="IOF7" pad="AA5"/>
<connect gate="-F" pin="IOF8" pad="AA39"/>
<connect gate="-F" pin="IOF9" pad="AB4"/>
<connect gate="-G" pin="IOG1" pad="AE1"/>
<connect gate="-G" pin="IOG10" pad="AD2"/>
<connect gate="-G" pin="IOG11" pad="AD4"/>
<connect gate="-G" pin="IOG12" pad="AD6"/>
<connect gate="-G" pin="IOG13" pad="AD42"/>
<connect gate="-G" pin="IOG14" pad="AE3"/>
<connect gate="-G" pin="IOG15" pad="AE7"/>
<connect gate="-G" pin="IOG16" pad="AF4"/>
<connect gate="-G" pin="IOG2" pad="AF2"/>
<connect gate="-G" pin="IOG3" pad="AC43"/>
<connect gate="-G" pin="IOG4" pad="AA43"/>
<connect gate="-G" pin="IOG5" pad="AB38"/>
<connect gate="-G" pin="IOG6" pad="AB40"/>
<connect gate="-G" pin="IOG7" pad="AB42"/>
<connect gate="-G" pin="IOG8" pad="AC37"/>
<connect gate="-G" pin="IOG9" pad="AC39"/>
<connect gate="-H" pin="IOH1" pad="AG3"/>
<connect gate="-H" pin="IOH10" pad="AF40"/>
<connect gate="-H" pin="IOH11" pad="AF42"/>
<connect gate="-H" pin="IOH12" pad="AG1"/>
<connect gate="-H" pin="IOH13" pad="AG5"/>
<connect gate="-H" pin="IOH14" pad="AG43"/>
<connect gate="-H" pin="IOH15" pad="AH4"/>
<connect gate="-H" pin="IOH16" pad="AJ1"/>
<connect gate="-H" pin="IOH2" pad="AH2"/>
<connect gate="-H" pin="IOH3" pad="AH6"/>
<connect gate="-H" pin="IOH4" pad="AE37"/>
<connect gate="-H" pin="IOH5" pad="AD40"/>
<connect gate="-H" pin="IOH6" pad="AD38"/>
<connect gate="-H" pin="IOH7" pad="AE41"/>
<connect gate="-H" pin="IOH8" pad="AE43"/>
<connect gate="-H" pin="IOH9" pad="AF6"/>
<connect gate="-I" pin="IOI1" pad="AJ5"/>
<connect gate="-I" pin="IOI10" pad="AK2"/>
<connect gate="-I" pin="IOI11" pad="AK4"/>
<connect gate="-I" pin="IOI12" pad="AK6"/>
<connect gate="-I" pin="IOI13" pad="AK42"/>
<connect gate="-I" pin="IOI14" pad="AL1"/>
<connect gate="-I" pin="IOI15" pad="AL3"/>
<connect gate="-I" pin="IOI16" pad="AM2"/>
<connect gate="-I" pin="IOI2" pad="AJ7"/>
<connect gate="-I" pin="IOI3" pad="AH40"/>
<connect gate="-I" pin="IOI4" pad="AF38"/>
<connect gate="-I" pin="IOI5" pad="AG39"/>
<connect gate="-I" pin="IOI6" pad="AG41"/>
<connect gate="-I" pin="IOI7" pad="AH38"/>
<connect gate="-I" pin="IOI8" pad="AH42"/>
<connect gate="-I" pin="IOI9" pad="AJ43"/>
<connect gate="-J" pin="IOJ1" pad="AP2"/>
<connect gate="-J" pin="IOJ10" pad="AM6"/>
<connect gate="-J" pin="IOJ11" pad="AM40"/>
<connect gate="-J" pin="IOJ12" pad="AM42"/>
<connect gate="-J" pin="IOJ13" pad="AN1"/>
<connect gate="-J" pin="IOJ14" pad="AN43"/>
<connect gate="-J" pin="IOJ15" pad="AP4"/>
<connect gate="-J" pin="IOJ16" pad="AR1"/>
<connect gate="-J" pin="IOJ2" pad="AN5"/>
<connect gate="-J" pin="IOJ3" pad="AK38"/>
<connect gate="-J" pin="IOJ4" pad="AJ37"/>
<connect gate="-J" pin="IOJ5" pad="AJ39"/>
<connect gate="-J" pin="IOJ6" pad="AK40"/>
<connect gate="-J" pin="IOJ7" pad="AL7"/>
<connect gate="-J" pin="IOJ8" pad="AL43"/>
<connect gate="-J" pin="IOJ9" pad="AM4"/>
<connect gate="-K" pin="IOK1" pad="AR5"/>
<connect gate="-K" pin="IOK10" pad="AR43"/>
<connect gate="-K" pin="IOK11" pad="AT2"/>
<connect gate="-K" pin="IOK12" pad="AT42"/>
<connect gate="-K" pin="IOK13" pad="AU1"/>
<connect gate="-K" pin="IOK14" pad="AU43"/>
<connect gate="-K" pin="IOK15" pad="AV2"/>
<connect gate="-K" pin="IOK16" pad="AW1"/>
<connect gate="-K" pin="IOK2" pad="AR7"/>
<connect gate="-K" pin="IOK3" pad="AN39"/>
<connect gate="-K" pin="IOK4" pad="AL37"/>
<connect gate="-K" pin="IOK5" pad="AM38"/>
<connect gate="-K" pin="IOK6" pad="AN7"/>
<connect gate="-K" pin="IOK7" pad="AP6"/>
<connect gate="-K" pin="IOK8" pad="AP40"/>
<connect gate="-K" pin="IOK9" pad="AP42"/>
<connect gate="-L" pin="IOL1" pad="AY2"/>
<connect gate="-L" pin="IOL10" pad="AT6"/>
<connect gate="-L" pin="IOL11" pad="AT38"/>
<connect gate="-L" pin="IOL12" pad="AU5"/>
<connect gate="-L" pin="IOL13" pad="AU39"/>
<connect gate="-L" pin="IOL14" pad="BA1"/>
<connect gate="-L" pin="IOL15" pad="BA3"/>
<connect gate="-L" pin="IOL16" pad="BB2"/>
<connect gate="-L" pin="IOL2" pad="BC1"/>
<connect gate="-L" pin="IOL3" pad="AV6"/>
<connect gate="-L" pin="IOL4" pad="AW43"/>
<connect gate="-L" pin="IOL5" pad="AV42"/>
<connect gate="-L" pin="IOL6" pad="AN37"/>
<connect gate="-L" pin="IOL7" pad="AP38"/>
<connect gate="-L" pin="IOL8" pad="AR37"/>
<connect gate="-L" pin="IOL9" pad="AR39"/>
<connect gate="1" pin="VCC" pad="AC3"/>
<connect gate="10" pin="VCC" pad="C11"/>
<connect gate="11" pin="VCC" pad="E39"/>
<connect gate="12" pin="VCC" pad="G27"/>
<connect gate="13" pin="VCC" pad="N5"/>
<connect gate="14" pin="VCC" pad="N41"/>
<connect gate="15" pin="VCC" pad="W39"/>
<connect gate="16" pin="VCCIO" pad="W5"/>
<connect gate="17" pin="VCCIO" pad="AC41"/>
<connect gate="18" pin="VCCIO" pad="AE5"/>
<connect gate="19" pin="VCCIO" pad="AJ41"/>
<connect gate="2" pin="VCC" pad="AG7"/>
<connect gate="20" pin="VCCIO" pad="AL39"/>
<connect gate="21" pin="VCCIO" pad="AU3"/>
<connect gate="22" pin="VCCIO" pad="AU17"/>
<connect gate="23" pin="VCCIO" pad="AW3"/>
<connect gate="24" pin="VCCIO" pad="AW19"/>
<connect gate="25" pin="VCCIO" pad="BA9"/>
<connect gate="26" pin="VCCIO" pad="BA27"/>
<connect gate="27" pin="VCCIO" pad="BA29"/>
<connect gate="28" pin="VCCIO" pad="BA37"/>
<connect gate="29" pin="VCCIO" pad="C9"/>
<connect gate="3" pin="VCC" pad="AR3"/>
<connect gate="30" pin="VCCIO" pad="C15"/>
<connect gate="31" pin="VCCIO" pad="C25"/>
<connect gate="32" pin="VCCIO" pad="C33"/>
<connect gate="33" pin="VCCIO" pad="C37"/>
<connect gate="34" pin="VCCIO" pad="E19"/>
<connect gate="35" pin="VCCIO" pad="E41"/>
<connect gate="36" pin="VCCIO" pad="G7"/>
<connect gate="37" pin="VCCIO" pad="L3"/>
<connect gate="38" pin="VCCIO" pad="R41"/>
<connect gate="39" pin="VCCIO" pad="U3"/>
<connect gate="4" pin="VCC" pad="AR41"/>
<connect gate="40" pin="VCCIO" pad="U37"/>
<connect gate="41" pin="GND" pad="AA3"/>
<connect gate="42" pin="GND" pad="AE39"/>
<connect gate="43" pin="GND" pad="AL5"/>
<connect gate="44" pin="GND" pad="AL41"/>
<connect gate="45" pin="GND" pad="AU27"/>
<connect gate="46" pin="GND" pad="AW39"/>
<connect gate="47" pin="GND" pad="BA7"/>
<connect gate="48" pin="GND" pad="BA13"/>
<connect gate="49" pin="GND" pad="C17"/>
<connect gate="5" pin="VCC" pad="AU37"/>
<connect gate="50" pin="GND" pad="E3"/>
<connect gate="51" pin="GND" pad="E5"/>
<connect gate="52" pin="GND" pad="E25"/>
<connect gate="53" pin="GND" pad="G37"/>
<connect gate="54" pin="GND" pad="J3"/>
<connect gate="55" pin="GND" pad="J41"/>
<connect gate="56" pin="GND" pad="U7"/>
<connect gate="58" pin="GNDIO" pad="AA41"/>
<connect gate="59" pin="GNDIO" pad="AG37"/>
<connect gate="6" pin="VCC" pad="AW5"/>
<connect gate="60" pin="GNDIO" pad="AJ3"/>
<connect gate="61" pin="GNDIO" pad="AN3"/>
<connect gate="62" pin="GNDIO" pad="AN41"/>
<connect gate="63" pin="GNDIO" pad="AU7"/>
<connect gate="64" pin="GNDIO" pad="AU41"/>
<connect gate="65" pin="GNDIO" pad="AW13"/>
<connect gate="66" pin="GNDIO" pad="AW31"/>
<connect gate="67" pin="GNDIO" pad="BA11"/>
<connect gate="68" pin="GNDIO" pad="BA21"/>
<connect gate="69" pin="GNDIO" pad="BA23"/>
<connect gate="7" pin="VCC" pad="AW25"/>
<connect gate="70" pin="GNDIO" pad="C21"/>
<connect gate="71" pin="GNDIO" pad="C23"/>
<connect gate="72" pin="GNDIO" pad="C39"/>
<connect gate="73" pin="GNDIO" pad="C41"/>
<connect gate="74" pin="GNDIO" pad="E13"/>
<connect gate="75" pin="GNDIO" pad="E31"/>
<connect gate="76" pin="GNDIO" pad="G3"/>
<connect gate="77" pin="GNDIO" pad="G17"/>
<connect gate="78" pin="GNDIO" pad="N3"/>
<connect gate="79" pin="GNDIO" pad="N39"/>
<connect gate="8" pin="VCC" pad="AW41"/>
<connect gate="80" pin="GNDIO" pad="R3"/>
<connect gate="81" pin="GNDIO" pad="W3"/>
<connect gate="82" pin="GNDIO" pad="W41"/>
<connect gate="9" pin="VCC" pad="BA17"/>
<connect gate="_" pin="/CE" pad="K40"/>
<connect gate="_" pin="/CEO" pad="H4"/>
<connect gate="_" pin="/CONFIG" pad="AY40"/>
<connect gate="_" pin="/STATUS" pad="AY4"/>
<connect gate="_" pin="CONF_DONE" pad="F4"/>
<connect gate="_" pin="DATA0" pad="F40"/>
<connect gate="_" pin="DCLK" pad="H40"/>
<connect gate="_" pin="GCLK0" pad="AY22"/>
<connect gate="_" pin="GCLK1" pad="D22"/>
<connect gate="_" pin="GND_CKLK" pad="BA25"/>
<connect gate="_" pin="IN0" pad="AY20"/>
<connect gate="_" pin="IN1" pad="AY24"/>
<connect gate="_" pin="IN2" pad="D24"/>
<connect gate="_" pin="IN3" pad="D20"/>
<connect gate="_" pin="MSEL0" pad="AT40"/>
<connect gate="_" pin="MSEL1" pad="AV40"/>
<connect gate="_" pin="TCK" pad="D4"/>
<connect gate="_" pin="TDI" pad="M40"/>
<connect gate="_" pin="TDO" pad="K4"/>
<connect gate="_" pin="TMS" pad="AT4"/>
<connect gate="_" pin="TRST" pad="AV4"/>
<connect gate="_" pin="VCC_CKLK" pad="BA19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K100A-R240" prefix="IC">
<description>&lt;b&gt;EPF10K100&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A10-100R"/>
<gate name="-B" symbol="B16-9"/>
<gate name="-C" symbol="C16-9"/>
<gate name="-D" symbol="D7-7"/>
<gate name="-E" symbol="E11-6"/>
<gate name="-F" symbol="F7-6"/>
<gate name="-G" symbol="G11-6"/>
<gate name="-H" symbol="H8-6"/>
<gate name="-I" symbol="I12-6"/>
<gate name="-J" symbol="J14-6"/>
<gate name="-K" symbol="K14-6"/>
<gate name="-L" symbol="L11-6"/>
<gate name="-1" symbol="122-100R"/>
<gate name="-2" symbol="192-100R"/>
<gate name="-3" symbol="261-100R"/>
<gate name="-4" symbol="323-100R"/>
<gate name="-5" symbol="411-100R"/>
<gate name="-6" symbol="502-100R"/>
<gate name="-7" symbol="522-100R"/>
<gate name="1" symbol="VCC"/>
<gate name="2" symbol="VCC"/>
<gate name="3" symbol="VCC"/>
<gate name="4" symbol="VCC"/>
<gate name="5" symbol="VCC"/>
<gate name="6" symbol="VCC"/>
<gate name="7" symbol="VCC"/>
<gate name="8" symbol="VCC"/>
<gate name="9" symbol="VCC"/>
<gate name="10" symbol="VCC"/>
<gate name="11" symbol="VCC"/>
<gate name="12" symbol="VCC"/>
<gate name="13" symbol="VCC"/>
<gate name="14" symbol="VCC"/>
<gate name="15" symbol="VCC"/>
<gate name="16" symbol="VCC"/>
<gate name="17" symbol="VCC"/>
<gate name="18" symbol="VCC"/>
<gate name="19" symbol="VCC"/>
<gate name="20" symbol="GND"/>
<gate name="21" symbol="GND"/>
<gate name="22" symbol="GND"/>
<gate name="23" symbol="GND"/>
<gate name="24" symbol="GND"/>
<gate name="25" symbol="GND"/>
<gate name="26" symbol="GND"/>
<gate name="27" symbol="GND"/>
<gate name="28" symbol="GND"/>
<gate name="29" symbol="GND"/>
<gate name="30" symbol="GND"/>
<gate name="31" symbol="GND"/>
<gate name="32" symbol="GND"/>
<gate name="33" symbol="GND"/>
<gate name="34" symbol="GND"/>
<gate name="35" symbol="GND"/>
<gate name="36" symbol="GND"/>
<gate name="37" symbol="GND"/>
</gates>
<devices>
<device name="" package="RQFP240">
<connects>
<connect gate="-1" pin="IO101" pad="182"/>
<connect gate="-1" pin="IO102" pad="110"/>
<connect gate="-1" pin="IO11" pad="120"/>
<connect gate="-1" pin="IO111" pad="183"/>
<connect gate="-1" pin="IO113" pad="109"/>
<connect gate="-1" pin="IO121" pad="184"/>
<connect gate="-1" pin="IO122" pad="185"/>
<connect gate="-1" pin="IO21" pad="119"/>
<connect gate="-1" pin="IO31" pad="118"/>
<connect gate="-1" pin="IO41" pad="117"/>
<connect gate="-1" pin="IO51" pad="116"/>
<connect gate="-1" pin="IO61" pad="115"/>
<connect gate="-1" pin="IO71" pad="114"/>
<connect gate="-1" pin="IO81" pad="113"/>
<connect gate="-1" pin="IO91" pad="111"/>
<connect gate="-1" pin="IO92" pad="181"/>
<connect gate="-2" pin="IO124" pad="108"/>
<connect gate="-2" pin="IO131" pad="107"/>
<connect gate="-2" pin="IO132" pad="186"/>
<connect gate="-2" pin="IO141" pad="106"/>
<connect gate="-2" pin="IO142" pad="187"/>
<connect gate="-2" pin="IO143" pad="188"/>
<connect gate="-2" pin="IO151" pad="105"/>
<connect gate="-2" pin="IO152" pad="190"/>
<connect gate="-2" pin="IO161" pad="103"/>
<connect gate="-2" pin="IO162" pad="192"/>
<connect gate="-2" pin="IO164" pad="191"/>
<connect gate="-2" pin="IO171" pad="193"/>
<connect gate="-2" pin="IO181" pad="102"/>
<connect gate="-2" pin="IO182" pad="194"/>
<connect gate="-2" pin="IO191" pad="101"/>
<connect gate="-2" pin="IO192" pad="196"/>
<connect gate="-3" pin="IO194" pad="195"/>
<connect gate="-3" pin="IO201" pad="198"/>
<connect gate="-3" pin="IO202" pad="100"/>
<connect gate="-3" pin="IO211" pad="99"/>
<connect gate="-3" pin="IO212" pad="199"/>
<connect gate="-3" pin="IO221" pad="200"/>
<connect gate="-3" pin="IO222" pad="201"/>
<connect gate="-3" pin="IO231" pad="98"/>
<connect gate="-3" pin="IO232" pad="203"/>
<connect gate="-3" pin="IO234" pad="202"/>
<connect gate="-3" pin="IO241" pad="97"/>
<connect gate="-3" pin="IO242" pad="204"/>
<connect gate="-3" pin="IO251" pad="95"/>
<connect gate="-3" pin="IO252" pad="207"/>
<connect gate="-3" pin="IO253" pad="206"/>
<connect gate="-3" pin="IO261" pad="209"/>
<connect gate="-4" pin="IO263" pad="208"/>
<connect gate="-4" pin="IO264" pad="94"/>
<connect gate="-4" pin="IO271" pad="87"/>
<connect gate="-4" pin="IO272" pad="213"/>
<connect gate="-4" pin="IO273" pad="88"/>
<connect gate="-4" pin="IO281" pad="86"/>
<connect gate="-4" pin="IO282" pad="214"/>
<connect gate="-4" pin="IO284" pad="215"/>
<connect gate="-4" pin="IO291" pad="83"/>
<connect gate="-4" pin="IO293" pad="84"/>
<connect gate="-4" pin="IO294" pad="217"/>
<connect gate="-4" pin="IO301" pad="82"/>
<connect gate="-4" pin="IO302" pad="218"/>
<connect gate="-4" pin="IO311" pad="81"/>
<connect gate="-4" pin="IO321" pad="80"/>
<connect gate="-4" pin="IO323" pad="219"/>
<connect gate="-5" pin="IO331" pad="78"/>
<connect gate="-5" pin="IO332" pad="79"/>
<connect gate="-5" pin="IO333" pad="220"/>
<connect gate="-5" pin="IO341" pad="76"/>
<connect gate="-5" pin="IO351" pad="74"/>
<connect gate="-5" pin="IO352" pad="75"/>
<connect gate="-5" pin="IO353" pad="221"/>
<connect gate="-5" pin="IO361" pad="73"/>
<connect gate="-5" pin="IO371" pad="222"/>
<connect gate="-5" pin="IO381" pad="223"/>
<connect gate="-5" pin="IO383" pad="72"/>
<connect gate="-5" pin="IO391" pad="225"/>
<connect gate="-5" pin="IO401" pad="70"/>
<connect gate="-5" pin="IO402" pad="71"/>
<connect gate="-5" pin="IO404" pad="226"/>
<connect gate="-5" pin="IO411" pad="227"/>
<connect gate="-6" pin="IO421" pad="68"/>
<connect gate="-6" pin="IO423" pad="228"/>
<connect gate="-6" pin="IO431" pad="67"/>
<connect gate="-6" pin="IO432" pad="229"/>
<connect gate="-6" pin="IO441" pad="230"/>
<connect gate="-6" pin="IO451" pad="66"/>
<connect gate="-6" pin="IO452" pad="231"/>
<connect gate="-6" pin="IO461" pad="233"/>
<connect gate="-6" pin="IO462" pad="65"/>
<connect gate="-6" pin="IO471" pad="234"/>
<connect gate="-6" pin="IO481" pad="64"/>
<connect gate="-6" pin="IO482" pad="235"/>
<connect gate="-6" pin="IO491" pad="236"/>
<connect gate="-6" pin="IO492" pad="63"/>
<connect gate="-6" pin="IO501" pad="237"/>
<connect gate="-6" pin="IO502" pad="238"/>
<connect gate="-7" pin="IO511" pad="62"/>
<connect gate="-7" pin="IO512" pad="239"/>
<connect gate="-7" pin="IO521" pad="61"/>
<connect gate="-7" pin="IO522" pad="240"/>
<connect gate="-A" pin="IOA1" pad="6"/>
<connect gate="-A" pin="IOA10" pad="9"/>
<connect gate="-A" pin="IOA2" pad="7"/>
<connect gate="-A" pin="IOA3" pad="8"/>
<connect gate="-A" pin="IOA4" pad="11"/>
<connect gate="-A" pin="IOA5" pad="171"/>
<connect gate="-A" pin="IOA6" pad="173"/>
<connect gate="-A" pin="IOA7" pad="175"/>
<connect gate="-A" pin="IOA8" pad="174"/>
<connect gate="-A" pin="IOA9" pad="172"/>
<connect gate="-B" pin="IOB1" pad="12"/>
<connect gate="-B" pin="IOB16" pad="14"/>
<connect gate="-B" pin="IOB2" pad="13"/>
<connect gate="-B" pin="IOB3" pad="15"/>
<connect gate="-B" pin="IOB5" pad="164"/>
<connect gate="-B" pin="IOB6" pad="166"/>
<connect gate="-B" pin="IOB7" pad="169"/>
<connect gate="-B" pin="IOB8" pad="168"/>
<connect gate="-B" pin="IOB9" pad="167"/>
<connect gate="-C" pin="IOC1" pad="19"/>
<connect gate="-C" pin="IOC11" pad="17"/>
<connect gate="-C" pin="IOC16" pad="20"/>
<connect gate="-C" pin="IOC2" pad="21"/>
<connect gate="-C" pin="IOC3" pad="159"/>
<connect gate="-C" pin="IOC4" pad="161"/>
<connect gate="-C" pin="IOC5" pad="162"/>
<connect gate="-C" pin="IOC6" pad="163"/>
<connect gate="-C" pin="IOC9" pad="18"/>
<connect gate="-D" pin="IOD1" pad="23"/>
<connect gate="-D" pin="IOD2" pad="24"/>
<connect gate="-D" pin="IOD3" pad="25"/>
<connect gate="-D" pin="IOD4" pad="26"/>
<connect gate="-D" pin="IOD5" pad="156"/>
<connect gate="-D" pin="IOD6" pad="157"/>
<connect gate="-D" pin="IOD7" pad="158"/>
<connect gate="-E" pin="IOE1" pad="29"/>
<connect gate="-E" pin="IOE11" pad="28"/>
<connect gate="-E" pin="IOE2" pad="30"/>
<connect gate="-E" pin="IOE3" pad="152"/>
<connect gate="-E" pin="IOE4" pad="153"/>
<connect gate="-E" pin="IOE5" pad="154"/>
<connect gate="-F" pin="IOF1" pad="33"/>
<connect gate="-F" pin="IOF2" pad="34"/>
<connect gate="-F" pin="IOF3" pad="148"/>
<connect gate="-F" pin="IOF4" pad="149"/>
<connect gate="-F" pin="IOF5" pad="151"/>
<connect gate="-F" pin="IOF7" pad="31"/>
<connect gate="-G" pin="IOG1" pad="36"/>
<connect gate="-G" pin="IOG11" pad="35"/>
<connect gate="-G" pin="IOG2" pad="38"/>
<connect gate="-G" pin="IOG3" pad="146"/>
<connect gate="-G" pin="IOG4" pad="147"/>
<connect gate="-G" pin="IOG8" pad="144"/>
<connect gate="-H" pin="IOH1" pad="39"/>
<connect gate="-H" pin="IOH2" pad="40"/>
<connect gate="-H" pin="IOH3" pad="41"/>
<connect gate="-H" pin="IOH4" pad="141"/>
<connect gate="-H" pin="IOH5" pad="143"/>
<connect gate="-H" pin="IOH8" pad="142"/>
<connect gate="-I" pin="IOI1" pad="43"/>
<connect gate="-I" pin="IOI12" pad="45"/>
<connect gate="-I" pin="IOI2" pad="44"/>
<connect gate="-I" pin="IOI3" pad="137"/>
<connect gate="-I" pin="IOI4" pad="139"/>
<connect gate="-I" pin="IOI5" pad="138"/>
<connect gate="-J" pin="IOJ1" pad="48"/>
<connect gate="-J" pin="IOJ13" pad="46"/>
<connect gate="-J" pin="IOJ14" pad="133"/>
<connect gate="-J" pin="IOJ2" pad="49"/>
<connect gate="-J" pin="IOJ3" pad="134"/>
<connect gate="-J" pin="IOJ5" pad="136"/>
<connect gate="-K" pin="IOK1" pad="51"/>
<connect gate="-K" pin="IOK11" pad="50"/>
<connect gate="-K" pin="IOK14" pad="129"/>
<connect gate="-K" pin="IOK2" pad="53"/>
<connect gate="-K" pin="IOK3" pad="131"/>
<connect gate="-K" pin="IOK4" pad="132"/>
<connect gate="-L" pin="IOL1" pad="54"/>
<connect gate="-L" pin="IOL11" pad="126"/>
<connect gate="-L" pin="IOL2" pad="55"/>
<connect gate="-L" pin="IOL3" pad="56"/>
<connect gate="-L" pin="IOL4" pad="127"/>
<connect gate="-L" pin="IOL5" pad="128"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="10" pin="VCC" pad="112"/>
<connect gate="11" pin="VCC" pad="122"/>
<connect gate="12" pin="VCC" pad="130"/>
<connect gate="13" pin="VCC" pad="140"/>
<connect gate="14" pin="VCC" pad="150"/>
<connect gate="15" pin="VCC" pad="160"/>
<connect gate="16" pin="VCC" pad="170"/>
<connect gate="17" pin="VCC" pad="189"/>
<connect gate="18" pin="VCC" pad="205"/>
<connect gate="19" pin="VCC" pad="224"/>
<connect gate="2" pin="VCC" pad="16"/>
<connect gate="20" pin="GND" pad="10"/>
<connect gate="21" pin="GND" pad="22"/>
<connect gate="22" pin="GND" pad="32"/>
<connect gate="23" pin="GND" pad="42"/>
<connect gate="24" pin="GND" pad="52"/>
<connect gate="25" pin="GND" pad="69"/>
<connect gate="26" pin="GND" pad="85"/>
<connect gate="27" pin="GND" pad="93"/>
<connect gate="28" pin="GND" pad="104"/>
<connect gate="29" pin="GND" pad="125"/>
<connect gate="3" pin="VCC" pad="27"/>
<connect gate="30" pin="GND" pad="135"/>
<connect gate="31" pin="GND" pad="145"/>
<connect gate="32" pin="GND" pad="155"/>
<connect gate="33" pin="GND" pad="165"/>
<connect gate="34" pin="GND" pad="176"/>
<connect gate="35" pin="GND" pad="197"/>
<connect gate="36" pin="GND" pad="216"/>
<connect gate="37" pin="GND" pad="232"/>
<connect gate="4" pin="VCC" pad="37"/>
<connect gate="5" pin="VCC" pad="47"/>
<connect gate="6" pin="VCC" pad="57"/>
<connect gate="7" pin="VCC" pad="77"/>
<connect gate="8" pin="VCC" pad="89"/>
<connect gate="9" pin="VCC" pad="96"/>
<connect gate="_" pin="/CE" pad="178"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="121"/>
<connect gate="_" pin="/STATUS" pad="60"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="180"/>
<connect gate="_" pin="DCLK" pad="179"/>
<connect gate="_" pin="GCLK0" pad="91"/>
<connect gate="_" pin="GCLK1" pad="211"/>
<connect gate="_" pin="IN0" pad="90"/>
<connect gate="_" pin="IN1" pad="92"/>
<connect gate="_" pin="IN2" pad="210"/>
<connect gate="_" pin="IN3" pad="212"/>
<connect gate="_" pin="MSEL0" pad="124"/>
<connect gate="_" pin="MSEL1" pad="123"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="177"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="58"/>
<connect gate="_" pin="TRST" pad="59"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K100ARC240-3N"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8800"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K100A-P240" prefix="IC">
<description>&lt;b&gt;EPF10K100&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A10-10"/>
<gate name="-B" symbol="B16-100"/>
<gate name="-C" symbol="C16-100"/>
<gate name="-DE" symbol="D7E11"/>
<gate name="-FG" symbol="F7G11"/>
<gate name="-HI" symbol="H8I12"/>
<gate name="-JK" symbol="J14K14"/>
<gate name="-L" symbol="L11-100"/>
<gate name="-1" symbol="122-100R"/>
<gate name="-2" symbol="192-100R"/>
<gate name="-3" symbol="261-100R"/>
<gate name="-4" symbol="323-100R"/>
<gate name="-5" symbol="411-100R"/>
<gate name="-6" symbol="502-100R"/>
<gate name="-7" symbol="522-100R"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCIO"/>
<gate name="10" symbol="VCCIO"/>
<gate name="11" symbol="VCCIO"/>
<gate name="12" symbol="VCCIO"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="20" symbol="GND"/>
<gate name="21" symbol="GND"/>
<gate name="22" symbol="GND"/>
<gate name="23" symbol="GND"/>
<gate name="24" symbol="GND"/>
<gate name="25" symbol="GND"/>
<gate name="26" symbol="GND"/>
<gate name="27" symbol="GND"/>
<gate name="28" symbol="GND"/>
<gate name="29" symbol="GND"/>
<gate name="30" symbol="GND"/>
<gate name="31" symbol="GND"/>
<gate name="32" symbol="GND"/>
<gate name="33" symbol="GND"/>
<gate name="34" symbol="GND"/>
<gate name="35" symbol="GND"/>
<gate name="36" symbol="GND"/>
<gate name="37" symbol="GND"/>
<gate name="19" symbol="VCC"/>
</gates>
<devices>
<device name="" package="PQFP240">
<connects>
<connect gate="-1" pin="IO101" pad="182"/>
<connect gate="-1" pin="IO102" pad="110"/>
<connect gate="-1" pin="IO11" pad="120"/>
<connect gate="-1" pin="IO111" pad="183"/>
<connect gate="-1" pin="IO113" pad="109"/>
<connect gate="-1" pin="IO121" pad="184"/>
<connect gate="-1" pin="IO122" pad="185"/>
<connect gate="-1" pin="IO21" pad="119"/>
<connect gate="-1" pin="IO31" pad="118"/>
<connect gate="-1" pin="IO41" pad="117"/>
<connect gate="-1" pin="IO51" pad="116"/>
<connect gate="-1" pin="IO61" pad="115"/>
<connect gate="-1" pin="IO71" pad="114"/>
<connect gate="-1" pin="IO81" pad="113"/>
<connect gate="-1" pin="IO91" pad="111"/>
<connect gate="-1" pin="IO92" pad="181"/>
<connect gate="-2" pin="IO124" pad="108"/>
<connect gate="-2" pin="IO131" pad="107"/>
<connect gate="-2" pin="IO132" pad="186"/>
<connect gate="-2" pin="IO141" pad="106"/>
<connect gate="-2" pin="IO142" pad="187"/>
<connect gate="-2" pin="IO143" pad="188"/>
<connect gate="-2" pin="IO151" pad="105"/>
<connect gate="-2" pin="IO152" pad="190"/>
<connect gate="-2" pin="IO161" pad="103"/>
<connect gate="-2" pin="IO162" pad="192"/>
<connect gate="-2" pin="IO164" pad="191"/>
<connect gate="-2" pin="IO171" pad="193"/>
<connect gate="-2" pin="IO181" pad="102"/>
<connect gate="-2" pin="IO182" pad="194"/>
<connect gate="-2" pin="IO191" pad="101"/>
<connect gate="-2" pin="IO192" pad="196"/>
<connect gate="-3" pin="IO194" pad="195"/>
<connect gate="-3" pin="IO201" pad="198"/>
<connect gate="-3" pin="IO202" pad="100"/>
<connect gate="-3" pin="IO211" pad="99"/>
<connect gate="-3" pin="IO212" pad="199"/>
<connect gate="-3" pin="IO221" pad="200"/>
<connect gate="-3" pin="IO222" pad="201"/>
<connect gate="-3" pin="IO231" pad="98"/>
<connect gate="-3" pin="IO232" pad="203"/>
<connect gate="-3" pin="IO234" pad="202"/>
<connect gate="-3" pin="IO241" pad="97"/>
<connect gate="-3" pin="IO242" pad="204"/>
<connect gate="-3" pin="IO251" pad="95"/>
<connect gate="-3" pin="IO252" pad="207"/>
<connect gate="-3" pin="IO253" pad="206"/>
<connect gate="-3" pin="IO261" pad="209"/>
<connect gate="-4" pin="IO263" pad="208"/>
<connect gate="-4" pin="IO264" pad="94"/>
<connect gate="-4" pin="IO271" pad="87"/>
<connect gate="-4" pin="IO272" pad="213"/>
<connect gate="-4" pin="IO273" pad="88"/>
<connect gate="-4" pin="IO281" pad="86"/>
<connect gate="-4" pin="IO282" pad="214"/>
<connect gate="-4" pin="IO284" pad="215"/>
<connect gate="-4" pin="IO291" pad="83"/>
<connect gate="-4" pin="IO293" pad="84"/>
<connect gate="-4" pin="IO294" pad="217"/>
<connect gate="-4" pin="IO301" pad="82"/>
<connect gate="-4" pin="IO302" pad="218"/>
<connect gate="-4" pin="IO311" pad="81"/>
<connect gate="-4" pin="IO321" pad="80"/>
<connect gate="-4" pin="IO323" pad="219"/>
<connect gate="-5" pin="IO331" pad="78"/>
<connect gate="-5" pin="IO332" pad="79"/>
<connect gate="-5" pin="IO333" pad="220"/>
<connect gate="-5" pin="IO341" pad="76"/>
<connect gate="-5" pin="IO351" pad="74"/>
<connect gate="-5" pin="IO352" pad="75"/>
<connect gate="-5" pin="IO353" pad="221"/>
<connect gate="-5" pin="IO361" pad="73"/>
<connect gate="-5" pin="IO371" pad="222"/>
<connect gate="-5" pin="IO381" pad="223"/>
<connect gate="-5" pin="IO383" pad="72"/>
<connect gate="-5" pin="IO391" pad="225"/>
<connect gate="-5" pin="IO401" pad="70"/>
<connect gate="-5" pin="IO402" pad="71"/>
<connect gate="-5" pin="IO404" pad="226"/>
<connect gate="-5" pin="IO411" pad="227"/>
<connect gate="-6" pin="IO421" pad="68"/>
<connect gate="-6" pin="IO423" pad="228"/>
<connect gate="-6" pin="IO431" pad="67"/>
<connect gate="-6" pin="IO432" pad="229"/>
<connect gate="-6" pin="IO441" pad="230"/>
<connect gate="-6" pin="IO451" pad="66"/>
<connect gate="-6" pin="IO452" pad="231"/>
<connect gate="-6" pin="IO461" pad="233"/>
<connect gate="-6" pin="IO462" pad="65"/>
<connect gate="-6" pin="IO471" pad="234"/>
<connect gate="-6" pin="IO481" pad="64"/>
<connect gate="-6" pin="IO482" pad="235"/>
<connect gate="-6" pin="IO491" pad="236"/>
<connect gate="-6" pin="IO492" pad="63"/>
<connect gate="-6" pin="IO501" pad="237"/>
<connect gate="-6" pin="IO502" pad="238"/>
<connect gate="-7" pin="IO511" pad="62"/>
<connect gate="-7" pin="IO512" pad="239"/>
<connect gate="-7" pin="IO521" pad="61"/>
<connect gate="-7" pin="IO522" pad="240"/>
<connect gate="-A" pin="IOA1" pad="6"/>
<connect gate="-A" pin="IOA10" pad="9"/>
<connect gate="-A" pin="IOA2" pad="7"/>
<connect gate="-A" pin="IOA3" pad="8"/>
<connect gate="-A" pin="IOA4" pad="11"/>
<connect gate="-A" pin="IOA5" pad="171"/>
<connect gate="-A" pin="IOA6" pad="173"/>
<connect gate="-A" pin="IOA7" pad="175"/>
<connect gate="-A" pin="IOA8" pad="174"/>
<connect gate="-A" pin="IOA9" pad="172"/>
<connect gate="-B" pin="IOB1" pad="12"/>
<connect gate="-B" pin="IOB16" pad="14"/>
<connect gate="-B" pin="IOB2" pad="13"/>
<connect gate="-B" pin="IOB3" pad="15"/>
<connect gate="-B" pin="IOB5" pad="164"/>
<connect gate="-B" pin="IOB6" pad="166"/>
<connect gate="-B" pin="IOB7" pad="169"/>
<connect gate="-B" pin="IOB8" pad="168"/>
<connect gate="-B" pin="IOB9" pad="167"/>
<connect gate="-C" pin="IOC1" pad="19"/>
<connect gate="-C" pin="IOC11" pad="17"/>
<connect gate="-C" pin="IOC16" pad="20"/>
<connect gate="-C" pin="IOC2" pad="21"/>
<connect gate="-C" pin="IOC3" pad="159"/>
<connect gate="-C" pin="IOC4" pad="161"/>
<connect gate="-C" pin="IOC5" pad="162"/>
<connect gate="-C" pin="IOC6" pad="163"/>
<connect gate="-C" pin="IOC9" pad="18"/>
<connect gate="-DE" pin="IOD1" pad="23"/>
<connect gate="-DE" pin="IOD2" pad="24"/>
<connect gate="-DE" pin="IOD3" pad="25"/>
<connect gate="-DE" pin="IOD4" pad="26"/>
<connect gate="-DE" pin="IOD5" pad="156"/>
<connect gate="-DE" pin="IOD6" pad="157"/>
<connect gate="-DE" pin="IOD7" pad="158"/>
<connect gate="-DE" pin="IOE1" pad="29"/>
<connect gate="-DE" pin="IOE11" pad="28"/>
<connect gate="-DE" pin="IOE2" pad="30"/>
<connect gate="-DE" pin="IOE3" pad="152"/>
<connect gate="-DE" pin="IOE4" pad="153"/>
<connect gate="-DE" pin="IOE5" pad="154"/>
<connect gate="-FG" pin="IOF1" pad="33"/>
<connect gate="-FG" pin="IOF2" pad="34"/>
<connect gate="-FG" pin="IOF3" pad="148"/>
<connect gate="-FG" pin="IOF4" pad="149"/>
<connect gate="-FG" pin="IOF5" pad="151"/>
<connect gate="-FG" pin="IOF7" pad="31"/>
<connect gate="-FG" pin="IOG1" pad="36"/>
<connect gate="-FG" pin="IOG11" pad="35"/>
<connect gate="-FG" pin="IOG2" pad="38"/>
<connect gate="-FG" pin="IOG3" pad="146"/>
<connect gate="-FG" pin="IOG4" pad="147"/>
<connect gate="-FG" pin="IOG8" pad="144"/>
<connect gate="-HI" pin="IOH1" pad="39"/>
<connect gate="-HI" pin="IOH2" pad="40"/>
<connect gate="-HI" pin="IOH3" pad="41"/>
<connect gate="-HI" pin="IOH4" pad="141"/>
<connect gate="-HI" pin="IOH5" pad="143"/>
<connect gate="-HI" pin="IOH8" pad="142"/>
<connect gate="-HI" pin="IOI1" pad="43"/>
<connect gate="-HI" pin="IOI12" pad="45"/>
<connect gate="-HI" pin="IOI2" pad="44"/>
<connect gate="-HI" pin="IOI3" pad="137"/>
<connect gate="-HI" pin="IOI4" pad="139"/>
<connect gate="-HI" pin="IOI5" pad="138"/>
<connect gate="-JK" pin="IOJ1" pad="48"/>
<connect gate="-JK" pin="IOJ13" pad="46"/>
<connect gate="-JK" pin="IOJ14" pad="133"/>
<connect gate="-JK" pin="IOJ2" pad="49"/>
<connect gate="-JK" pin="IOJ3" pad="134"/>
<connect gate="-JK" pin="IOJ5" pad="136"/>
<connect gate="-JK" pin="IOK1" pad="51"/>
<connect gate="-JK" pin="IOK11" pad="50"/>
<connect gate="-JK" pin="IOK14" pad="129"/>
<connect gate="-JK" pin="IOK2" pad="53"/>
<connect gate="-JK" pin="IOK3" pad="131"/>
<connect gate="-JK" pin="IOK4" pad="132"/>
<connect gate="-L" pin="IOL1" pad="54"/>
<connect gate="-L" pin="IOL11" pad="126"/>
<connect gate="-L" pin="IOL2" pad="55"/>
<connect gate="-L" pin="IOL3" pad="56"/>
<connect gate="-L" pin="IOL4" pad="127"/>
<connect gate="-L" pin="IOL5" pad="128"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="10" pin="VCCIO" pad="16"/>
<connect gate="11" pin="VCCIO" pad="37"/>
<connect gate="12" pin="VCCIO" pad="57"/>
<connect gate="13" pin="VCCIO" pad="77"/>
<connect gate="14" pin="VCCIO" pad="112"/>
<connect gate="15" pin="VCCIO" pad="140"/>
<connect gate="16" pin="VCCIO" pad="160"/>
<connect gate="17" pin="VCCIO" pad="189"/>
<connect gate="18" pin="VCCIO" pad="205"/>
<connect gate="19" pin="VCC" pad="224"/>
<connect gate="2" pin="VCC" pad="27"/>
<connect gate="20" pin="GND" pad="10"/>
<connect gate="21" pin="GND" pad="22"/>
<connect gate="22" pin="GND" pad="32"/>
<connect gate="23" pin="GND" pad="42"/>
<connect gate="24" pin="GND" pad="52"/>
<connect gate="25" pin="GND" pad="69"/>
<connect gate="26" pin="GND" pad="85"/>
<connect gate="27" pin="GND" pad="93"/>
<connect gate="28" pin="GND" pad="104"/>
<connect gate="29" pin="GND" pad="125"/>
<connect gate="3" pin="VCC" pad="47"/>
<connect gate="30" pin="GND" pad="135"/>
<connect gate="31" pin="GND" pad="145"/>
<connect gate="32" pin="GND" pad="155"/>
<connect gate="33" pin="GND" pad="165"/>
<connect gate="34" pin="GND" pad="176"/>
<connect gate="35" pin="GND" pad="197"/>
<connect gate="36" pin="GND" pad="216"/>
<connect gate="37" pin="GND" pad="232"/>
<connect gate="4" pin="VCC" pad="89"/>
<connect gate="5" pin="VCC" pad="96"/>
<connect gate="6" pin="VCC" pad="122"/>
<connect gate="7" pin="VCC" pad="130"/>
<connect gate="8" pin="VCC" pad="150"/>
<connect gate="9" pin="VCCIO" pad="170"/>
<connect gate="_" pin="/CE" pad="178"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="121"/>
<connect gate="_" pin="/STATUS" pad="60"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="180"/>
<connect gate="_" pin="DCLK" pad="179"/>
<connect gate="_" pin="GCLK0" pad="91"/>
<connect gate="_" pin="GCLK1" pad="211"/>
<connect gate="_" pin="IN0" pad="90"/>
<connect gate="_" pin="IN1" pad="92"/>
<connect gate="_" pin="IN2" pad="210"/>
<connect gate="_" pin="IN3" pad="212"/>
<connect gate="_" pin="MSEL0" pad="124"/>
<connect gate="_" pin="MSEL1" pad="123"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="177"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="58"/>
<connect gate="_" pin="TRST" pad="59"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K100ARC240-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8795"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K100-P208" prefix="IC">
<description>&lt;b&gt;EPF10K100&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100P208C"/>
<gate name="-AB" symbol="A7B7"/>
<gate name="-CD" symbol="C6D7"/>
<gate name="-EFG" symbol="E4F4G4"/>
<gate name="-HIJ" symbol="H5I3J3"/>
<gate name="-KL" symbol="K4L5"/>
<gate name="-1" symbol="132-208"/>
<gate name="-2" symbol="221-208"/>
<gate name="-3" symbol="311-208"/>
<gate name="-4" symbol="421-208"/>
<gate name="-5" symbol="522-208"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCIO"/>
<gate name="12" symbol="VCCIO"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="19" symbol="VCCIO"/>
<gate name="20" symbol="VCCIO"/>
<gate name="21" symbol="VCCIO"/>
<gate name="22" symbol="VCCIO"/>
<gate name="23" symbol="VCCIO"/>
<gate name="24" symbol="VCCIO"/>
<gate name="25" symbol="GNDINT"/>
<gate name="26" symbol="GNDINT"/>
<gate name="27" symbol="GNDINT"/>
<gate name="28" symbol="GNDINT"/>
<gate name="29" symbol="GNDINT"/>
<gate name="30" symbol="GNDINT"/>
<gate name="31" symbol="GNDINT"/>
<gate name="32" symbol="GNDINT"/>
<gate name="33" symbol="GNDIO"/>
<gate name="34" symbol="GNDIO"/>
<gate name="35" symbol="GNDIO"/>
<gate name="36" symbol="GNDIO"/>
<gate name="37" symbol="GNDIO"/>
<gate name="38" symbol="GNDIO"/>
<gate name="39" symbol="GNDIO"/>
<gate name="40" symbol="GNDIO"/>
<gate name="41" symbol="GNDIO"/>
<gate name="42" symbol="GNDIO"/>
<gate name="43" symbol="GNDIO"/>
<gate name="44" symbol="GNDIO"/>
<gate name="45" symbol="VCCINT"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="-1" pin="IO101" pad="158"/>
<connect gate="-1" pin="IO11" pad="104"/>
<connect gate="-1" pin="IO111" pad="159"/>
<connect gate="-1" pin="IO121" pad="160"/>
<connect gate="-1" pin="IO122" pad="161"/>
<connect gate="-1" pin="IO131" pad="94"/>
<connect gate="-1" pin="IO132" pad="162"/>
<connect gate="-1" pin="IO21" pad="103"/>
<connect gate="-1" pin="IO31" pad="102"/>
<connect gate="-1" pin="IO41" pad="101"/>
<connect gate="-1" pin="IO51" pad="100"/>
<connect gate="-1" pin="IO61" pad="99"/>
<connect gate="-1" pin="IO71" pad="97"/>
<connect gate="-1" pin="IO81" pad="96"/>
<connect gate="-1" pin="IO91" pad="95"/>
<connect gate="-1" pin="IO92" pad="157"/>
<connect gate="-2" pin="IO141" pad="93"/>
<connect gate="-2" pin="IO142" pad="163"/>
<connect gate="-2" pin="IO143" pad="164"/>
<connect gate="-2" pin="IO151" pad="92"/>
<connect gate="-2" pin="IO152" pad="166"/>
<connect gate="-2" pin="IO161" pad="90"/>
<connect gate="-2" pin="IO162" pad="167"/>
<connect gate="-2" pin="IO171" pad="168"/>
<connect gate="-2" pin="IO181" pad="89"/>
<connect gate="-2" pin="IO182" pad="169"/>
<connect gate="-2" pin="IO191" pad="88"/>
<connect gate="-2" pin="IO192" pad="170"/>
<connect gate="-2" pin="IO201" pad="172"/>
<connect gate="-2" pin="IO211" pad="87"/>
<connect gate="-2" pin="IO212" pad="173"/>
<connect gate="-2" pin="IO221" pad="174"/>
<connect gate="-3" pin="IO222" pad="175"/>
<connect gate="-3" pin="IO231" pad="86"/>
<connect gate="-3" pin="IO232" pad="176"/>
<connect gate="-3" pin="IO241" pad="85"/>
<connect gate="-3" pin="IO242" pad="177"/>
<connect gate="-3" pin="IO251" pad="83"/>
<connect gate="-3" pin="IO252" pad="179"/>
<connect gate="-3" pin="IO261" pad="180"/>
<connect gate="-3" pin="IO271" pad="75"/>
<connect gate="-3" pin="IO272" pad="186"/>
<connect gate="-3" pin="IO281" pad="74"/>
<connect gate="-3" pin="IO282" pad="187"/>
<connect gate="-3" pin="IO291" pad="73"/>
<connect gate="-3" pin="IO301" pad="71"/>
<connect gate="-3" pin="IO302" pad="189"/>
<connect gate="-3" pin="IO311" pad="70"/>
<connect gate="-4" pin="IO321" pad="69"/>
<connect gate="-4" pin="IO331" pad="67"/>
<connect gate="-4" pin="IO332" pad="68"/>
<connect gate="-4" pin="IO333" pad="190"/>
<connect gate="-4" pin="IO341" pad="65"/>
<connect gate="-4" pin="IO351" pad="63"/>
<connect gate="-4" pin="IO352" pad="64"/>
<connect gate="-4" pin="IO353" pad="191"/>
<connect gate="-4" pin="IO361" pad="62"/>
<connect gate="-4" pin="IO371" pad="192"/>
<connect gate="-4" pin="IO381" pad="193"/>
<connect gate="-4" pin="IO391" pad="195"/>
<connect gate="-4" pin="IO401" pad="60"/>
<connect gate="-4" pin="IO402" pad="61"/>
<connect gate="-4" pin="IO411" pad="196"/>
<connect gate="-4" pin="IO421" pad="58"/>
<connect gate="-5" pin="IO431" pad="57"/>
<connect gate="-5" pin="IO432" pad="197"/>
<connect gate="-5" pin="IO441" pad="198"/>
<connect gate="-5" pin="IO451" pad="56"/>
<connect gate="-5" pin="IO452" pad="199"/>
<connect gate="-5" pin="IO461" pad="200"/>
<connect gate="-5" pin="IO471" pad="202"/>
<connect gate="-5" pin="IO481" pad="55"/>
<connect gate="-5" pin="IO482" pad="203"/>
<connect gate="-5" pin="IO491" pad="204"/>
<connect gate="-5" pin="IO501" pad="205"/>
<connect gate="-5" pin="IO502" pad="206"/>
<connect gate="-5" pin="IO511" pad="54"/>
<connect gate="-5" pin="IO512" pad="207"/>
<connect gate="-5" pin="IO521" pad="53"/>
<connect gate="-5" pin="IO522" pad="208"/>
<connect gate="-AB" pin="IOA1" pad="7"/>
<connect gate="-AB" pin="IOA2" pad="8"/>
<connect gate="-AB" pin="IOA3" pad="9"/>
<connect gate="-AB" pin="IOA4" pad="10"/>
<connect gate="-AB" pin="IOA5" pad="148"/>
<connect gate="-AB" pin="IOA6" pad="149"/>
<connect gate="-AB" pin="IOA7" pad="150"/>
<connect gate="-AB" pin="IOB1" pad="11"/>
<connect gate="-AB" pin="IOB2" pad="12"/>
<connect gate="-AB" pin="IOB3" pad="13"/>
<connect gate="-AB" pin="IOB4" pad="142"/>
<connect gate="-AB" pin="IOB5" pad="143"/>
<connect gate="-AB" pin="IOB6" pad="144"/>
<connect gate="-AB" pin="IOB7" pad="147"/>
<connect gate="-CD" pin="IOC1" pad="14"/>
<connect gate="-CD" pin="IOC2" pad="15"/>
<connect gate="-CD" pin="IOC3" pad="136"/>
<connect gate="-CD" pin="IOC4" pad="139"/>
<connect gate="-CD" pin="IOC5" pad="140"/>
<connect gate="-CD" pin="IOC6" pad="141"/>
<connect gate="-CD" pin="IOD1" pad="16"/>
<connect gate="-CD" pin="IOD2" pad="17"/>
<connect gate="-CD" pin="IOD3" pad="18"/>
<connect gate="-CD" pin="IOD4" pad="19"/>
<connect gate="-CD" pin="IOD5" pad="133"/>
<connect gate="-CD" pin="IOD6" pad="134"/>
<connect gate="-CD" pin="IOD7" pad="135"/>
<connect gate="-EFG" pin="IOE1" pad="24"/>
<connect gate="-EFG" pin="IOE2" pad="25"/>
<connect gate="-EFG" pin="IOE3" pad="128"/>
<connect gate="-EFG" pin="IOE4" pad="131"/>
<connect gate="-EFG" pin="IOE5" pad="132"/>
<connect gate="-EFG" pin="IOF1" pad="26"/>
<connect gate="-EFG" pin="IOF2" pad="27"/>
<connect gate="-EFG" pin="IOF3" pad="125"/>
<connect gate="-EFG" pin="IOF4" pad="126"/>
<connect gate="-EFG" pin="IOF5" pad="127"/>
<connect gate="-EFG" pin="IOG1" pad="28"/>
<connect gate="-EFG" pin="IOG2" pad="29"/>
<connect gate="-EFG" pin="IOG3" pad="121"/>
<connect gate="-EFG" pin="IOG4" pad="122"/>
<connect gate="-HIJ" pin="IOH1" pad="30"/>
<connect gate="-HIJ" pin="IOH2" pad="31"/>
<connect gate="-HIJ" pin="IOH3" pad="36"/>
<connect gate="-HIJ" pin="IOH4" pad="119"/>
<connect gate="-HIJ" pin="IOH5" pad="120"/>
<connect gate="-HIJ" pin="IOI1" pad="37"/>
<connect gate="-HIJ" pin="IOI2" pad="38"/>
<connect gate="-HIJ" pin="IOI3" pad="116"/>
<connect gate="-HIJ" pin="IOJ1" pad="39"/>
<connect gate="-HIJ" pin="IOJ2" pad="40"/>
<connect gate="-HIJ" pin="IOJ3" pad="115"/>
<connect gate="-KL" pin="IOK1" pad="41"/>
<connect gate="-KL" pin="IOK2" pad="44"/>
<connect gate="-KL" pin="IOK3" pad="113"/>
<connect gate="-KL" pin="IOK4" pad="114"/>
<connect gate="-KL" pin="IOL1" pad="45"/>
<connect gate="-KL" pin="IOL2" pad="46"/>
<connect gate="-KL" pin="IOL3" pad="47"/>
<connect gate="-KL" pin="IOL4" pad="111"/>
<connect gate="-KL" pin="IOL5" pad="112"/>
<connect gate="1" pin="VCC" pad="6"/>
<connect gate="10" pin="VCC" pad="145"/>
<connect gate="11" pin="VCCIO" pad="5"/>
<connect gate="12" pin="VCCIO" pad="22"/>
<connect gate="13" pin="VCCIO" pad="34"/>
<connect gate="14" pin="VCCIO" pad="42"/>
<connect gate="15" pin="VCCIO" pad="66"/>
<connect gate="16" pin="VCCIO" pad="84"/>
<connect gate="17" pin="VCCIO" pad="98"/>
<connect gate="18" pin="VCCIO" pad="110"/>
<connect gate="19" pin="VCCIO" pad="118"/>
<connect gate="2" pin="VCC" pad="23"/>
<connect gate="20" pin="VCCIO" pad="138"/>
<connect gate="21" pin="VCCIO" pad="146"/>
<connect gate="22" pin="VCCIO" pad="165"/>
<connect gate="23" pin="VCCIO" pad="178"/>
<connect gate="24" pin="VCCIO" pad="194"/>
<connect gate="25" pin="GND" pad="21"/>
<connect gate="26" pin="GND" pad="33"/>
<connect gate="27" pin="GND" pad="49"/>
<connect gate="28" pin="GND" pad="81"/>
<connect gate="29" pin="GND" pad="82"/>
<connect gate="3" pin="VCC" pad="35"/>
<connect gate="30" pin="GND" pad="123"/>
<connect gate="31" pin="GND" pad="129"/>
<connect gate="32" pin="GND" pad="151"/>
<connect gate="33" pin="GNDIO" pad="20"/>
<connect gate="34" pin="GNDIO" pad="32"/>
<connect gate="35" pin="GNDIO" pad="48"/>
<connect gate="36" pin="GNDIO" pad="59"/>
<connect gate="37" pin="GNDIO" pad="72"/>
<connect gate="38" pin="GNDIO" pad="91"/>
<connect gate="39" pin="GNDIO" pad="124"/>
<connect gate="4" pin="VCC" pad="43"/>
<connect gate="40" pin="GNDIO" pad="130"/>
<connect gate="41" pin="GNDIO" pad="152"/>
<connect gate="42" pin="GNDIO" pad="171"/>
<connect gate="43" pin="GNDIO" pad="188"/>
<connect gate="44" pin="GNDIO" pad="201"/>
<connect gate="45" pin="VCC" pad="181"/>
<connect gate="5" pin="VCC" pad="76"/>
<connect gate="6" pin="VCC" pad="77"/>
<connect gate="7" pin="VCC" pad="106"/>
<connect gate="8" pin="VCC" pad="109"/>
<connect gate="9" pin="VCC" pad="117"/>
<connect gate="_" pin="/CE" pad="154"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="105"/>
<connect gate="_" pin="/STATUS" pad="52"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="156"/>
<connect gate="_" pin="DCLK" pad="155"/>
<connect gate="_" pin="GCLK0" pad="79"/>
<connect gate="_" pin="GCLK1" pad="183"/>
<connect gate="_" pin="GND_CKLK" pad="185"/>
<connect gate="_" pin="IN0" pad="78"/>
<connect gate="_" pin="IN1" pad="80"/>
<connect gate="_" pin="IN2" pad="182"/>
<connect gate="_" pin="IN3" pad="184"/>
<connect gate="_" pin="MSEL0" pad="108"/>
<connect gate="_" pin="MSEL1" pad="107"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="153"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="50"/>
<connect gate="_" pin="TRST" pad="51"/>
<connect gate="_" pin="VCC_CKLK" pad="137"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K100EQC208-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8827"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K40-P240" prefix="IC">
<description>&lt;b&gt;EPF10K40&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A11"/>
<gate name="-B" symbol="B10"/>
<gate name="-C" symbol="C11_4"/>
<gate name="-D" symbol="D11"/>
<gate name="-E" symbol="E10"/>
<gate name="-F" symbol="F10"/>
<gate name="-G" symbol="G11"/>
<gate name="-H" symbol="H11"/>
<gate name="-1" symbol="63-40"/>
<gate name="-2" symbol="122-40"/>
<gate name="-3" symbol="181-40"/>
<gate name="-4" symbol="232-40"/>
<gate name="-5" symbol="292-40"/>
<gate name="-6" symbol="351-40"/>
<gate name="-7" symbol="363-40"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCINT"/>
<gate name="14" symbol="VCCINT"/>
<gate name="15" symbol="VCCINT"/>
<gate name="16" symbol="VCCINT"/>
<gate name="17" symbol="VCCINT"/>
<gate name="18" symbol="VCCINT"/>
<gate name="19" symbol="VCCINT"/>
<gate name="20" symbol="GNDINT"/>
<gate name="21" symbol="GNDINT"/>
<gate name="22" symbol="GNDINT"/>
<gate name="23" symbol="GNDINT"/>
<gate name="24" symbol="GNDINT"/>
<gate name="25" symbol="GNDINT"/>
<gate name="26" symbol="GNDINT"/>
<gate name="27" symbol="GNDINT"/>
<gate name="28" symbol="GNDINT"/>
<gate name="29" symbol="GNDINT"/>
<gate name="30" symbol="GNDINT"/>
<gate name="31" symbol="GNDINT"/>
<gate name="32" symbol="GNDINT"/>
<gate name="33" symbol="GNDINT"/>
<gate name="34" symbol="GNDINT"/>
<gate name="35" symbol="GNDINT"/>
<gate name="36" symbol="GNDINT"/>
<gate name="37" symbol="GNDINT"/>
</gates>
<devices>
<device name="" package="PQFP240">
<connects>
<connect gate="-1" pin="IO11" pad="120"/>
<connect gate="-1" pin="IO12" pad="181"/>
<connect gate="-1" pin="IO21" pad="118"/>
<connect gate="-1" pin="IO22" pad="182"/>
<connect gate="-1" pin="IO23" pad="119"/>
<connect gate="-1" pin="IO31" pad="117"/>
<connect gate="-1" pin="IO32" pad="183"/>
<connect gate="-1" pin="IO41" pad="116"/>
<connect gate="-1" pin="IO42" pad="184"/>
<connect gate="-1" pin="IO43" pad="185"/>
<connect gate="-1" pin="IO51" pad="115"/>
<connect gate="-1" pin="IO52" pad="186"/>
<connect gate="-1" pin="IO53" pad="114"/>
<connect gate="-1" pin="IO61" pad="113"/>
<connect gate="-1" pin="IO62" pad="187"/>
<connect gate="-1" pin="IO63" pad="188"/>
<connect gate="-2" pin="IO101" pad="106"/>
<connect gate="-2" pin="IO102" pad="194"/>
<connect gate="-2" pin="IO111" pad="105"/>
<connect gate="-2" pin="IO112" pad="196"/>
<connect gate="-2" pin="IO113" pad="195"/>
<connect gate="-2" pin="IO121" pad="102"/>
<connect gate="-2" pin="IO122" pad="198"/>
<connect gate="-2" pin="IO71" pad="110"/>
<connect gate="-2" pin="IO72" pad="190"/>
<connect gate="-2" pin="IO73" pad="111"/>
<connect gate="-2" pin="IO81" pad="109"/>
<connect gate="-2" pin="IO82" pad="192"/>
<connect gate="-2" pin="IO83" pad="191"/>
<connect gate="-2" pin="IO91" pad="107"/>
<connect gate="-2" pin="IO92" pad="108"/>
<connect gate="-2" pin="IO93" pad="193"/>
<connect gate="-3" pin="IO123" pad="103"/>
<connect gate="-3" pin="IO131" pad="100"/>
<connect gate="-3" pin="IO132" pad="199"/>
<connect gate="-3" pin="IO133" pad="101"/>
<connect gate="-3" pin="IO141" pad="99"/>
<connect gate="-3" pin="IO143" pad="200"/>
<connect gate="-3" pin="IO144" pad="201"/>
<connect gate="-3" pin="IO151" pad="98"/>
<connect gate="-3" pin="IO152" pad="203"/>
<connect gate="-3" pin="IO153" pad="202"/>
<connect gate="-3" pin="IO161" pad="97"/>
<connect gate="-3" pin="IO162" pad="204"/>
<connect gate="-3" pin="IO171" pad="95"/>
<connect gate="-3" pin="IO172" pad="207"/>
<connect gate="-3" pin="IO173" pad="206"/>
<connect gate="-3" pin="IO181" pad="209"/>
<connect gate="-4" pin="IO182" pad="208"/>
<connect gate="-4" pin="IO183" pad="94"/>
<connect gate="-4" pin="IO191" pad="87"/>
<connect gate="-4" pin="IO192" pad="213"/>
<connect gate="-4" pin="IO193" pad="88"/>
<connect gate="-4" pin="IO201" pad="86"/>
<connect gate="-4" pin="IO203" pad="215"/>
<connect gate="-4" pin="IO204" pad="214"/>
<connect gate="-4" pin="IO211" pad="83"/>
<connect gate="-4" pin="IO212" pad="217"/>
<connect gate="-4" pin="IO213" pad="84"/>
<connect gate="-4" pin="IO221" pad="82"/>
<connect gate="-4" pin="IO222" pad="219"/>
<connect gate="-4" pin="IO223" pad="218"/>
<connect gate="-4" pin="IO231" pad="81"/>
<connect gate="-4" pin="IO232" pad="221"/>
<connect gate="-5" pin="IO233" pad="220"/>
<connect gate="-5" pin="IO241" pad="80"/>
<connect gate="-5" pin="IO242" pad="222"/>
<connect gate="-5" pin="IO251" pad="78"/>
<connect gate="-5" pin="IO252" pad="223"/>
<connect gate="-5" pin="IO253" pad="79"/>
<connect gate="-5" pin="IO261" pad="75"/>
<connect gate="-5" pin="IO262" pad="76"/>
<connect gate="-5" pin="IO263" pad="225"/>
<connect gate="-5" pin="IO271" pad="74"/>
<connect gate="-5" pin="IO272" pad="227"/>
<connect gate="-5" pin="IO273" pad="226"/>
<connect gate="-5" pin="IO281" pad="73"/>
<connect gate="-5" pin="IO283" pad="228"/>
<connect gate="-5" pin="IO291" pad="72"/>
<connect gate="-5" pin="IO292" pad="229"/>
<connect gate="-6" pin="IO293" pad="71"/>
<connect gate="-6" pin="IO301" pad="70"/>
<connect gate="-6" pin="IO302" pad="231"/>
<connect gate="-6" pin="IO303" pad="230"/>
<connect gate="-6" pin="IO311" pad="67"/>
<connect gate="-6" pin="IO312" pad="233"/>
<connect gate="-6" pin="IO313" pad="68"/>
<connect gate="-6" pin="IO321" pad="66"/>
<connect gate="-6" pin="IO322" pad="235"/>
<connect gate="-6" pin="IO323" pad="234"/>
<connect gate="-6" pin="IO331" pad="65"/>
<connect gate="-6" pin="IO332" pad="236"/>
<connect gate="-6" pin="IO341" pad="64"/>
<connect gate="-6" pin="IO342" pad="237"/>
<connect gate="-6" pin="IO343" pad="238"/>
<connect gate="-6" pin="IO351" pad="63"/>
<connect gate="-7" pin="IO352" pad="239"/>
<connect gate="-7" pin="IO361" pad="61"/>
<connect gate="-7" pin="IO362" pad="240"/>
<connect gate="-7" pin="IO363" pad="62"/>
<connect gate="-A" pin="IOA1" pad="6"/>
<connect gate="-A" pin="IOA10" pad="8"/>
<connect gate="-A" pin="IOA11" pad="172"/>
<connect gate="-A" pin="IOA2" pad="7"/>
<connect gate="-A" pin="IOA3" pad="9"/>
<connect gate="-A" pin="IOA4" pad="11"/>
<connect gate="-A" pin="IOA5" pad="169"/>
<connect gate="-A" pin="IOA6" pad="171"/>
<connect gate="-A" pin="IOA7" pad="174"/>
<connect gate="-A" pin="IOA8" pad="175"/>
<connect gate="-A" pin="IOA9" pad="173"/>
<connect gate="-B" pin="IOB1" pad="12"/>
<connect gate="-B" pin="IOB10" pad="13"/>
<connect gate="-B" pin="IOB2" pad="15"/>
<connect gate="-B" pin="IOB3" pad="17"/>
<connect gate="-B" pin="IOB4" pad="163"/>
<connect gate="-B" pin="IOB5" pad="164"/>
<connect gate="-B" pin="IOB6" pad="166"/>
<connect gate="-B" pin="IOB7" pad="168"/>
<connect gate="-B" pin="IOB8" pad="167"/>
<connect gate="-B" pin="IOB9" pad="14"/>
<connect gate="-C" pin="IOC1" pad="18"/>
<connect gate="-C" pin="IOC10" pad="19"/>
<connect gate="-C" pin="IOC11" pad="159"/>
<connect gate="-C" pin="IOC2" pad="20"/>
<connect gate="-C" pin="IOC3" pad="23"/>
<connect gate="-C" pin="IOC5" pad="157"/>
<connect gate="-C" pin="IOC6" pad="158"/>
<connect gate="-C" pin="IOC7" pad="161"/>
<connect gate="-C" pin="IOC8" pad="162"/>
<connect gate="-C" pin="IOC9" pad="21"/>
<connect gate="-D" pin="IOD1" pad="24"/>
<connect gate="-D" pin="IOD10" pad="154"/>
<connect gate="-D" pin="IOD11" pad="25"/>
<connect gate="-D" pin="IOD2" pad="26"/>
<connect gate="-D" pin="IOD3" pad="29"/>
<connect gate="-D" pin="IOD4" pad="30"/>
<connect gate="-D" pin="IOD5" pad="151"/>
<connect gate="-D" pin="IOD6" pad="152"/>
<connect gate="-D" pin="IOD7" pad="153"/>
<connect gate="-D" pin="IOD8" pad="156"/>
<connect gate="-D" pin="IOD9" pad="28"/>
<connect gate="-E" pin="IOE1" pad="31"/>
<connect gate="-E" pin="IOE10" pad="34"/>
<connect gate="-E" pin="IOE2" pad="33"/>
<connect gate="-E" pin="IOE3" pad="35"/>
<connect gate="-E" pin="IOE4" pad="36"/>
<connect gate="-E" pin="IOE5" pad="144"/>
<connect gate="-E" pin="IOE6" pad="146"/>
<connect gate="-E" pin="IOE7" pad="147"/>
<connect gate="-E" pin="IOE8" pad="149"/>
<connect gate="-E" pin="IOE9" pad="148"/>
<connect gate="-F" pin="IOF1" pad="38"/>
<connect gate="-F" pin="IOF10" pad="142"/>
<connect gate="-F" pin="IOF2" pad="39"/>
<connect gate="-F" pin="IOF3" pad="41"/>
<connect gate="-F" pin="IOF4" pad="43"/>
<connect gate="-F" pin="IOF5" pad="138"/>
<connect gate="-F" pin="IOF6" pad="139"/>
<connect gate="-F" pin="IOF7" pad="141"/>
<connect gate="-F" pin="IOF8" pad="143"/>
<connect gate="-F" pin="IOF9" pad="40"/>
<connect gate="-G" pin="IOG1" pad="44"/>
<connect gate="-G" pin="IOG10" pad="133"/>
<connect gate="-G" pin="IOG11" pad="136"/>
<connect gate="-G" pin="IOG2" pad="45"/>
<connect gate="-G" pin="IOG3" pad="46"/>
<connect gate="-G" pin="IOG5" pad="132"/>
<connect gate="-G" pin="IOG6" pad="134"/>
<connect gate="-G" pin="IOG7" pad="137"/>
<connect gate="-G" pin="IOG8" pad="49"/>
<connect gate="-G" pin="IOG9" pad="48"/>
<connect gate="-H" pin="IOH1" pad="50"/>
<connect gate="-H" pin="IOH10" pad="54"/>
<connect gate="-H" pin="IOH11" pad="51"/>
<connect gate="-H" pin="IOH2" pad="53"/>
<connect gate="-H" pin="IOH3" pad="55"/>
<connect gate="-H" pin="IOH4" pad="56"/>
<connect gate="-H" pin="IOH5" pad="126"/>
<connect gate="-H" pin="IOH6" pad="128"/>
<connect gate="-H" pin="IOH7" pad="131"/>
<connect gate="-H" pin="IOH8" pad="129"/>
<connect gate="-H" pin="IOH9" pad="127"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="10" pin="VCC" pad="112"/>
<connect gate="11" pin="VCC" pad="122"/>
<connect gate="12" pin="VCC" pad="130"/>
<connect gate="13" pin="VCC" pad="140"/>
<connect gate="14" pin="VCC" pad="150"/>
<connect gate="15" pin="VCC" pad="160"/>
<connect gate="16" pin="VCC" pad="170"/>
<connect gate="17" pin="VCC" pad="189"/>
<connect gate="18" pin="VCC" pad="205"/>
<connect gate="19" pin="VCC" pad="224"/>
<connect gate="2" pin="VCC" pad="16"/>
<connect gate="20" pin="GND" pad="10"/>
<connect gate="21" pin="GND" pad="22"/>
<connect gate="22" pin="GND" pad="32"/>
<connect gate="23" pin="GND" pad="42"/>
<connect gate="24" pin="GND" pad="52"/>
<connect gate="25" pin="GND" pad="69"/>
<connect gate="26" pin="GND" pad="85"/>
<connect gate="27" pin="GND" pad="93"/>
<connect gate="28" pin="GND" pad="104"/>
<connect gate="29" pin="GND" pad="125"/>
<connect gate="3" pin="VCC" pad="27"/>
<connect gate="30" pin="GND" pad="135"/>
<connect gate="31" pin="GND" pad="145"/>
<connect gate="32" pin="GND" pad="155"/>
<connect gate="33" pin="GND" pad="165"/>
<connect gate="34" pin="GND" pad="176"/>
<connect gate="35" pin="GND" pad="197"/>
<connect gate="36" pin="GND" pad="216"/>
<connect gate="37" pin="GND" pad="232"/>
<connect gate="4" pin="VCC" pad="37"/>
<connect gate="5" pin="VCC" pad="47"/>
<connect gate="6" pin="VCC" pad="57"/>
<connect gate="7" pin="VCC" pad="77"/>
<connect gate="8" pin="VCC" pad="89"/>
<connect gate="9" pin="VCC" pad="96"/>
<connect gate="_" pin="/CE" pad="178"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="121"/>
<connect gate="_" pin="/STATUS" pad="60"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="180"/>
<connect gate="_" pin="DCLK" pad="179"/>
<connect gate="_" pin="GCLK0" pad="91"/>
<connect gate="_" pin="GCLK1" pad="211"/>
<connect gate="_" pin="IN0" pad="90"/>
<connect gate="_" pin="IN1" pad="92"/>
<connect gate="_" pin="IN2" pad="210"/>
<connect gate="_" pin="IN3" pad="212"/>
<connect gate="_" pin="MSEL0" pad="124"/>
<connect gate="_" pin="MSEL1" pad="123"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="177"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="58"/>
<connect gate="_" pin="TRST" pad="59"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K40RC240-4N"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9017"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K40-R208" prefix="IC">
<description>&lt;b&gt;EPF10K40&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-AB" symbol="A8B7"/>
<gate name="-CD" symbol="C8D8"/>
<gate name="-EF" symbol="E8F8"/>
<gate name="-GH" symbol="G7H7"/>
<gate name="-1" symbol="72-40R"/>
<gate name="-2" symbol="143-40R"/>
<gate name="-3" symbol="221-40R"/>
<gate name="-4" symbol="291-40R"/>
<gate name="-5" symbol="362-40R"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="19" symbol="VCCIO"/>
<gate name="20" symbol="VCCIO"/>
<gate name="21" symbol="VCCIO"/>
<gate name="22" symbol="VCCIO"/>
<gate name="23" symbol="VCCIO"/>
<gate name="24" symbol="VCCIO"/>
<gate name="25" symbol="VCCIO"/>
<gate name="26" symbol="VCCIO"/>
<gate name="27" symbol="GNDINT"/>
<gate name="28" symbol="GNDINT"/>
<gate name="29" symbol="GNDINT"/>
<gate name="30" symbol="GNDINT"/>
<gate name="31" symbol="GNDINT"/>
<gate name="32" symbol="GNDINT"/>
<gate name="33" symbol="GNDINT"/>
<gate name="34" symbol="GNDINT"/>
<gate name="35" symbol="GNDINT"/>
<gate name="36" symbol="GNDIO"/>
<gate name="37" symbol="GNDIO"/>
<gate name="38" symbol="GNDIO"/>
<gate name="39" symbol="GNDIO"/>
<gate name="40" symbol="GNDIO"/>
<gate name="41" symbol="GNDIO"/>
<gate name="42" symbol="GNDIO"/>
<gate name="43" symbol="GNDIO"/>
<gate name="44" symbol="GNDIO"/>
<gate name="45" symbol="GNDIO"/>
<gate name="46" symbol="GNDIO"/>
<gate name="47" symbol="GNDIO"/>
</gates>
<devices>
<device name="" package="RQFP208">
<connects>
<connect gate="-1" pin="IO11" pad="104"/>
<connect gate="-1" pin="IO12" pad="157"/>
<connect gate="-1" pin="IO21" pad="103"/>
<connect gate="-1" pin="IO22" pad="158"/>
<connect gate="-1" pin="IO31" pad="102"/>
<connect gate="-1" pin="IO32" pad="159"/>
<connect gate="-1" pin="IO41" pad="101"/>
<connect gate="-1" pin="IO42" pad="160"/>
<connect gate="-1" pin="IO43" pad="161"/>
<connect gate="-1" pin="IO51" pad="100"/>
<connect gate="-1" pin="IO52" pad="162"/>
<connect gate="-1" pin="IO61" pad="99"/>
<connect gate="-1" pin="IO62" pad="163"/>
<connect gate="-1" pin="IO63" pad="164"/>
<connect gate="-1" pin="IO71" pad="97"/>
<connect gate="-1" pin="IO72" pad="166"/>
<connect gate="-2" pin="IO101" pad="93"/>
<connect gate="-2" pin="IO102" pad="169"/>
<connect gate="-2" pin="IO111" pad="92"/>
<connect gate="-2" pin="IO112" pad="170"/>
<connect gate="-2" pin="IO121" pad="90"/>
<connect gate="-2" pin="IO122" pad="172"/>
<connect gate="-2" pin="IO131" pad="89"/>
<connect gate="-2" pin="IO132" pad="173"/>
<connect gate="-2" pin="IO141" pad="87"/>
<connect gate="-2" pin="IO142" pad="88"/>
<connect gate="-2" pin="IO143" pad="174"/>
<connect gate="-2" pin="IO81" pad="96"/>
<connect gate="-2" pin="IO82" pad="167"/>
<connect gate="-2" pin="IO91" pad="94"/>
<connect gate="-2" pin="IO92" pad="95"/>
<connect gate="-2" pin="IO93" pad="168"/>
<connect gate="-3" pin="IO144" pad="175"/>
<connect gate="-3" pin="IO151" pad="86"/>
<connect gate="-3" pin="IO152" pad="176"/>
<connect gate="-3" pin="IO161" pad="85"/>
<connect gate="-3" pin="IO162" pad="177"/>
<connect gate="-3" pin="IO171" pad="83"/>
<connect gate="-3" pin="IO172" pad="179"/>
<connect gate="-3" pin="IO181" pad="180"/>
<connect gate="-3" pin="IO191" pad="75"/>
<connect gate="-3" pin="IO192" pad="186"/>
<connect gate="-3" pin="IO201" pad="73"/>
<connect gate="-3" pin="IO202" pad="74"/>
<connect gate="-3" pin="IO203" pad="187"/>
<connect gate="-3" pin="IO211" pad="71"/>
<connect gate="-3" pin="IO212" pad="189"/>
<connect gate="-3" pin="IO221" pad="70"/>
<connect gate="-4" pin="IO222" pad="190"/>
<connect gate="-4" pin="IO231" pad="69"/>
<connect gate="-4" pin="IO232" pad="191"/>
<connect gate="-4" pin="IO241" pad="68"/>
<connect gate="-4" pin="IO242" pad="192"/>
<connect gate="-4" pin="IO251" pad="67"/>
<connect gate="-4" pin="IO252" pad="193"/>
<connect gate="-4" pin="IO261" pad="64"/>
<connect gate="-4" pin="IO262" pad="65"/>
<connect gate="-4" pin="IO263" pad="195"/>
<connect gate="-4" pin="IO271" pad="63"/>
<connect gate="-4" pin="IO272" pad="196"/>
<connect gate="-4" pin="IO281" pad="62"/>
<connect gate="-4" pin="IO282" pad="197"/>
<connect gate="-4" pin="IO283" pad="198"/>
<connect gate="-4" pin="IO291" pad="61"/>
<connect gate="-5" pin="IO292" pad="199"/>
<connect gate="-5" pin="IO301" pad="60"/>
<connect gate="-5" pin="IO302" pad="200"/>
<connect gate="-5" pin="IO311" pad="58"/>
<connect gate="-5" pin="IO312" pad="202"/>
<connect gate="-5" pin="IO321" pad="57"/>
<connect gate="-5" pin="IO322" pad="203"/>
<connect gate="-5" pin="IO331" pad="56"/>
<connect gate="-5" pin="IO332" pad="204"/>
<connect gate="-5" pin="IO341" pad="55"/>
<connect gate="-5" pin="IO342" pad="205"/>
<connect gate="-5" pin="IO343" pad="206"/>
<connect gate="-5" pin="IO351" pad="54"/>
<connect gate="-5" pin="IO352" pad="207"/>
<connect gate="-5" pin="IO361" pad="53"/>
<connect gate="-5" pin="IO362" pad="208"/>
<connect gate="-AB" pin="IOA1" pad="7"/>
<connect gate="-AB" pin="IOA2" pad="8"/>
<connect gate="-AB" pin="IOA3" pad="9"/>
<connect gate="-AB" pin="IOA4" pad="10"/>
<connect gate="-AB" pin="IOA5" pad="147"/>
<connect gate="-AB" pin="IOA6" pad="148"/>
<connect gate="-AB" pin="IOA7" pad="149"/>
<connect gate="-AB" pin="IOA8" pad="150"/>
<connect gate="-AB" pin="IOB1" pad="11"/>
<connect gate="-AB" pin="IOB2" pad="12"/>
<connect gate="-AB" pin="IOB3" pad="13"/>
<connect gate="-AB" pin="IOB4" pad="141"/>
<connect gate="-AB" pin="IOB5" pad="142"/>
<connect gate="-AB" pin="IOB6" pad="143"/>
<connect gate="-AB" pin="IOB7" pad="144"/>
<connect gate="-CD" pin="IOC1" pad="14"/>
<connect gate="-CD" pin="IOC2" pad="15"/>
<connect gate="-CD" pin="IOC3" pad="16"/>
<connect gate="-CD" pin="IOC4" pad="17"/>
<connect gate="-CD" pin="IOC5" pad="135"/>
<connect gate="-CD" pin="IOC6" pad="136"/>
<connect gate="-CD" pin="IOC7" pad="139"/>
<connect gate="-CD" pin="IOC8" pad="140"/>
<connect gate="-CD" pin="IOD1" pad="18"/>
<connect gate="-CD" pin="IOD2" pad="19"/>
<connect gate="-CD" pin="IOD3" pad="24"/>
<connect gate="-CD" pin="IOD4" pad="25"/>
<connect gate="-CD" pin="IOD5" pad="131"/>
<connect gate="-CD" pin="IOD6" pad="132"/>
<connect gate="-CD" pin="IOD7" pad="133"/>
<connect gate="-CD" pin="IOD8" pad="134"/>
<connect gate="-EF" pin="IOE1" pad="26"/>
<connect gate="-EF" pin="IOE2" pad="27"/>
<connect gate="-EF" pin="IOE3" pad="28"/>
<connect gate="-EF" pin="IOE4" pad="29"/>
<connect gate="-EF" pin="IOE5" pad="125"/>
<connect gate="-EF" pin="IOE6" pad="126"/>
<connect gate="-EF" pin="IOE7" pad="127"/>
<connect gate="-EF" pin="IOE8" pad="128"/>
<connect gate="-EF" pin="IOF1" pad="30"/>
<connect gate="-EF" pin="IOF2" pad="31"/>
<connect gate="-EF" pin="IOF3" pad="36"/>
<connect gate="-EF" pin="IOF4" pad="37"/>
<connect gate="-EF" pin="IOF5" pad="119"/>
<connect gate="-EF" pin="IOF6" pad="120"/>
<connect gate="-EF" pin="IOF7" pad="121"/>
<connect gate="-EF" pin="IOF8" pad="122"/>
<connect gate="-GH" pin="IOG1" pad="38"/>
<connect gate="-GH" pin="IOG2" pad="39"/>
<connect gate="-GH" pin="IOG3" pad="40"/>
<connect gate="-GH" pin="IOG4" pad="41"/>
<connect gate="-GH" pin="IOG5" pad="114"/>
<connect gate="-GH" pin="IOG6" pad="115"/>
<connect gate="-GH" pin="IOG7" pad="116"/>
<connect gate="-GH" pin="IOH1" pad="44"/>
<connect gate="-GH" pin="IOH2" pad="45"/>
<connect gate="-GH" pin="IOH3" pad="46"/>
<connect gate="-GH" pin="IOH4" pad="47"/>
<connect gate="-GH" pin="IOH5" pad="111"/>
<connect gate="-GH" pin="IOH6" pad="112"/>
<connect gate="-GH" pin="IOH7" pad="113"/>
<connect gate="1" pin="VCC" pad="6"/>
<connect gate="10" pin="VCC" pad="137"/>
<connect gate="11" pin="VCC" pad="145"/>
<connect gate="12" pin="VCC" pad="181"/>
<connect gate="13" pin="VCCIO" pad="5"/>
<connect gate="14" pin="VCCIO" pad="22"/>
<connect gate="15" pin="VCCIO" pad="34"/>
<connect gate="16" pin="VCCIO" pad="42"/>
<connect gate="17" pin="VCCIO" pad="66"/>
<connect gate="18" pin="VCCIO" pad="84"/>
<connect gate="19" pin="VCCIO" pad="98"/>
<connect gate="2" pin="VCC" pad="23"/>
<connect gate="20" pin="VCCIO" pad="110"/>
<connect gate="21" pin="VCCIO" pad="118"/>
<connect gate="22" pin="VCCIO" pad="138"/>
<connect gate="23" pin="VCCIO" pad="146"/>
<connect gate="24" pin="VCCIO" pad="165"/>
<connect gate="25" pin="VCCIO" pad="178"/>
<connect gate="26" pin="VCCIO" pad="194"/>
<connect gate="27" pin="GND" pad="21"/>
<connect gate="28" pin="GND" pad="33"/>
<connect gate="29" pin="GND" pad="49"/>
<connect gate="3" pin="VCC" pad="35"/>
<connect gate="30" pin="GND" pad="81"/>
<connect gate="31" pin="GND" pad="82"/>
<connect gate="32" pin="GND" pad="123"/>
<connect gate="33" pin="GND" pad="129"/>
<connect gate="34" pin="GND" pad="151"/>
<connect gate="35" pin="GND" pad="185"/>
<connect gate="36" pin="GNDIO" pad="20"/>
<connect gate="37" pin="GNDIO" pad="32"/>
<connect gate="38" pin="GNDIO" pad="48"/>
<connect gate="39" pin="GNDIO" pad="59"/>
<connect gate="4" pin="VCC" pad="43"/>
<connect gate="40" pin="GNDIO" pad="72"/>
<connect gate="41" pin="GNDIO" pad="91"/>
<connect gate="42" pin="GNDIO" pad="124"/>
<connect gate="43" pin="GNDIO" pad="130"/>
<connect gate="44" pin="GNDIO" pad="152"/>
<connect gate="45" pin="GNDIO" pad="171"/>
<connect gate="46" pin="GNDIO" pad="188"/>
<connect gate="47" pin="GNDIO" pad="201"/>
<connect gate="5" pin="VCC" pad="76"/>
<connect gate="6" pin="VCC" pad="77"/>
<connect gate="7" pin="VCC" pad="106"/>
<connect gate="8" pin="VCC" pad="109"/>
<connect gate="9" pin="VCC" pad="117"/>
<connect gate="_" pin="/CE" pad="154"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="105"/>
<connect gate="_" pin="/STATUS" pad="52"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="156"/>
<connect gate="_" pin="DCLK" pad="155"/>
<connect gate="_" pin="GCLK0" pad="79"/>
<connect gate="_" pin="GCLK1" pad="183"/>
<connect gate="_" pin="IN0" pad="78"/>
<connect gate="_" pin="IN1" pad="80"/>
<connect gate="_" pin="IN2" pad="182"/>
<connect gate="_" pin="IN3" pad="184"/>
<connect gate="_" pin="MSEL0" pad="108"/>
<connect gate="_" pin="MSEL1" pad="107"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="153"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="50"/>
<connect gate="_" pin="TRST" pad="51"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K40RC208-3"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R9013"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30A-FGBA484" prefix="IC">
<description>&lt;b&gt;EPF10K30&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A12"/>
<gate name="-B" symbol="B11"/>
<gate name="-C" symbol="C12"/>
<gate name="-D" symbol="D12"/>
<gate name="-E" symbol="E11"/>
<gate name="-F" symbol="F12"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC40" symbol="NC"/>
<gate name="NC41" symbol="NC"/>
<gate name="NC42" symbol="NC"/>
<gate name="NC43" symbol="NC"/>
<gate name="NC44" symbol="NC"/>
<gate name="NC45" symbol="NC"/>
<gate name="NC46" symbol="NC"/>
<gate name="NC47" symbol="NC"/>
<gate name="NC48" symbol="NC"/>
<gate name="NC49" symbol="NC"/>
<gate name="NC50" symbol="NC"/>
<gate name="NC51" symbol="NC"/>
<gate name="NC52" symbol="NC"/>
<gate name="NC53" symbol="NC"/>
<gate name="NC54" symbol="NC"/>
<gate name="NC55" symbol="NC"/>
<gate name="NC56" symbol="NC"/>
<gate name="NC57" symbol="NC"/>
<gate name="NC58" symbol="NC"/>
<gate name="NC59" symbol="NC"/>
<gate name="NC60" symbol="NC"/>
<gate name="NC61" symbol="NC"/>
<gate name="NC62" symbol="NC"/>
<gate name="NC63" symbol="NC"/>
<gate name="NC64" symbol="NC"/>
<gate name="NC65" symbol="NC"/>
<gate name="NC66" symbol="NC"/>
<gate name="NC67" symbol="NC"/>
<gate name="NC68" symbol="NC"/>
<gate name="NC69" symbol="NC"/>
<gate name="NC70" symbol="NC"/>
<gate name="NC71" symbol="NC"/>
<gate name="NC72" symbol="NC"/>
<gate name="NC73" symbol="NC"/>
<gate name="NC74" symbol="NC"/>
<gate name="NC75" symbol="NC"/>
<gate name="NC76" symbol="NC"/>
<gate name="NC77" symbol="NC"/>
<gate name="NC78" symbol="NC"/>
<gate name="NC79" symbol="NC"/>
<gate name="NC80" symbol="NC"/>
<gate name="NC81" symbol="NC"/>
<gate name="NC82" symbol="NC"/>
<gate name="NC83" symbol="NC"/>
<gate name="NC84" symbol="NC"/>
<gate name="NC85" symbol="NC"/>
<gate name="NC86" symbol="NC"/>
<gate name="NC87" symbol="NC"/>
<gate name="NC88" symbol="NC"/>
<gate name="NC89" symbol="NC"/>
<gate name="NC90" symbol="NC"/>
<gate name="NC91" symbol="NC"/>
<gate name="NC92" symbol="NC"/>
<gate name="NC93" symbol="NC"/>
<gate name="NC94" symbol="NC"/>
<gate name="NC95" symbol="NC"/>
<gate name="NC96" symbol="NC"/>
<gate name="NC97" symbol="NC"/>
<gate name="NC98" symbol="NC"/>
<gate name="NC99" symbol="NC"/>
<gate name="NC100" symbol="NC"/>
<gate name="NC101" symbol="NC"/>
<gate name="NC102" symbol="NC"/>
<gate name="NC103" symbol="NC"/>
<gate name="NC104" symbol="NC"/>
<gate name="NC105" symbol="NC"/>
<gate name="NC106" symbol="NC"/>
<gate name="NC107" symbol="NC"/>
<gate name="NC108" symbol="NC"/>
<gate name="NC109" symbol="NC"/>
<gate name="NC110" symbol="NC"/>
<gate name="NC111" symbol="NC"/>
<gate name="NC112" symbol="NC"/>
<gate name="NC113" symbol="NC"/>
<gate name="NC114" symbol="NC"/>
<gate name="NC115" symbol="NC"/>
<gate name="NC116" symbol="NC"/>
<gate name="NC117" symbol="NC"/>
<gate name="NC118" symbol="NC"/>
<gate name="NC119" symbol="NC"/>
<gate name="NC120" symbol="NC"/>
<gate name="NC121" symbol="NC"/>
<gate name="NC122" symbol="NC"/>
<gate name="NC123" symbol="NC"/>
<gate name="NC124" symbol="NC"/>
<gate name="NC125" symbol="NC"/>
<gate name="NC126" symbol="NC"/>
<gate name="NC127" symbol="NC"/>
<gate name="NC128" symbol="NC"/>
<gate name="NC129" symbol="NC"/>
<gate name="NC130" symbol="NC"/>
<gate name="NC131" symbol="NC"/>
<gate name="NC132" symbol="NC"/>
<gate name="NC133" symbol="NC"/>
<gate name="NC134" symbol="NC"/>
<gate name="NC135" symbol="NC"/>
<gate name="NC136" symbol="NC"/>
<gate name="NC137" symbol="NC"/>
<gate name="NC138" symbol="NC"/>
<gate name="NC139" symbol="NC"/>
<gate name="NC140" symbol="NC"/>
<gate name="NC141" symbol="NC"/>
<gate name="NC142" symbol="NC"/>
<gate name="NC143" symbol="NC"/>
<gate name="NC144" symbol="NC"/>
<gate name="NC145" symbol="NC"/>
<gate name="NC146" symbol="NC"/>
<gate name="NC147" symbol="NC"/>
<gate name="NC148" symbol="NC"/>
<gate name="NC149" symbol="NC"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="FBGA484">
<connects>
<connect gate="-1" pin="IO11" pad="W4"/>
<connect gate="-1" pin="IO12" pad="E6"/>
<connect gate="-1" pin="IO13" pad="W3"/>
<connect gate="-1" pin="IO14" pad="C3"/>
<connect gate="-1" pin="IO21" pad="W6"/>
<connect gate="-1" pin="IO22" pad="D5"/>
<connect gate="-1" pin="IO23" pad="W5"/>
<connect gate="-1" pin="IO24" pad="C4"/>
<connect gate="-1" pin="IO31" pad="U6"/>
<connect gate="-1" pin="IO32" pad="F6"/>
<connect gate="-1" pin="IO33" pad="Y5"/>
<connect gate="-1" pin="IO34" pad="C5"/>
<connect gate="-1" pin="IO41" pad="V6"/>
<connect gate="-1" pin="IO42" pad="D6"/>
<connect gate="-1" pin="IO43" pad="E7"/>
<connect gate="-1" pin="IO44" pad="AA5"/>
<connect gate="-2" pin="IO51" pad="U7"/>
<connect gate="-2" pin="IO52" pad="D7"/>
<connect gate="-2" pin="IO53" pad="B6"/>
<connect gate="-2" pin="IO54" pad="Y6"/>
<connect gate="-2" pin="IO61" pad="W7"/>
<connect gate="-2" pin="IO62" pad="F7"/>
<connect gate="-2" pin="IO63" pad="G7"/>
<connect gate="-2" pin="IO64" pad="Y7"/>
<connect gate="-2" pin="IO71" pad="T8"/>
<connect gate="-2" pin="IO72" pad="E8"/>
<connect gate="-2" pin="IO73" pad="V7"/>
<connect gate="-2" pin="IO74" pad="C7"/>
<connect gate="-2" pin="IO81" pad="U8"/>
<connect gate="-2" pin="IO82" pad="D8"/>
<connect gate="-2" pin="IO83" pad="B7"/>
<connect gate="-2" pin="IO84" pad="AB6"/>
<connect gate="-3" pin="IO101" pad="T9"/>
<connect gate="-3" pin="IO102" pad="G8"/>
<connect gate="-3" pin="IO103" pad="V8"/>
<connect gate="-3" pin="IO104" pad="B8"/>
<connect gate="-3" pin="IO111" pad="U9"/>
<connect gate="-3" pin="IO112" pad="E9"/>
<connect gate="-3" pin="IO113" pad="H7"/>
<connect gate="-3" pin="IO114" pad="AA8"/>
<connect gate="-3" pin="IO121" pad="V9"/>
<connect gate="-3" pin="IO122" pad="F9"/>
<connect gate="-3" pin="IO123" pad="D9"/>
<connect gate="-3" pin="IO124" pad="W9"/>
<connect gate="-3" pin="IO91" pad="W8"/>
<connect gate="-3" pin="IO92" pad="AA7"/>
<connect gate="-3" pin="IO93" pad="F8"/>
<connect gate="-3" pin="IO94" pad="C8"/>
<connect gate="-4" pin="IO131" pad="T10"/>
<connect gate="-4" pin="IO132" pad="G9"/>
<connect gate="-4" pin="IO133" pad="R10"/>
<connect gate="-4" pin="IO134" pad="A10"/>
<connect gate="-4" pin="IO141" pad="W10"/>
<connect gate="-4" pin="IO142" pad="U10"/>
<connect gate="-4" pin="IO143" pad="D10"/>
<connect gate="-4" pin="IO144" pad="E10"/>
<connect gate="-4" pin="IO151" pad="V10"/>
<connect gate="-4" pin="IO152" pad="G10"/>
<connect gate="-4" pin="IO153" pad="F10"/>
<connect gate="-4" pin="IO154" pad="Y10"/>
<connect gate="-4" pin="IO161" pad="R11"/>
<connect gate="-4" pin="IO162" pad="H10"/>
<connect gate="-4" pin="IO163" pad="B11"/>
<connect gate="-4" pin="IO164" pad="AA10"/>
<connect gate="-5" pin="IO171" pad="T11"/>
<connect gate="-5" pin="IO172" pad="E11"/>
<connect gate="-5" pin="IO173" pad="D11"/>
<connect gate="-5" pin="IO174" pad="AB10"/>
<connect gate="-5" pin="IO181" pad="G11"/>
<connect gate="-5" pin="IO182" pad="F11"/>
<connect gate="-5" pin="IO183" pad="U11"/>
<connect gate="-5" pin="IO184" pad="Y11"/>
<connect gate="-5" pin="IO191" pad="W12"/>
<connect gate="-5" pin="IO192" pad="F12"/>
<connect gate="-5" pin="IO193" pad="V12"/>
<connect gate="-5" pin="IO194" pad="B13"/>
<connect gate="-5" pin="IO201" pad="T12"/>
<connect gate="-5" pin="IO202" pad="U12"/>
<connect gate="-5" pin="IO203" pad="H12"/>
<connect gate="-5" pin="IO204" pad="G12"/>
<connect gate="-6" pin="IO211" pad="V13"/>
<connect gate="-6" pin="IO212" pad="D13"/>
<connect gate="-6" pin="IO213" pad="U13"/>
<connect gate="-6" pin="IO214" pad="B14"/>
<connect gate="-6" pin="IO221" pad="W13"/>
<connect gate="-6" pin="IO222" pad="F13"/>
<connect gate="-6" pin="IO223" pad="E13"/>
<connect gate="-6" pin="IO224" pad="AB14"/>
<connect gate="-6" pin="IO231" pad="T13"/>
<connect gate="-6" pin="IO232" pad="H13"/>
<connect gate="-6" pin="IO233" pad="G13"/>
<connect gate="-6" pin="IO234" pad="AA14"/>
<connect gate="-6" pin="IO241" pad="R13"/>
<connect gate="-6" pin="IO242" pad="D14"/>
<connect gate="-6" pin="IO243" pad="B15"/>
<connect gate="-6" pin="IO244" pad="Y14"/>
<connect gate="-7" pin="IO251" pad="W14"/>
<connect gate="-7" pin="IO252" pad="E14"/>
<connect gate="-7" pin="IO253" pad="V14"/>
<connect gate="-7" pin="IO254" pad="A16"/>
<connect gate="-7" pin="IO261" pad="T14"/>
<connect gate="-7" pin="IO262" pad="U14"/>
<connect gate="-7" pin="IO263" pad="G14"/>
<connect gate="-7" pin="IO264" pad="F14"/>
<connect gate="-7" pin="IO271" pad="V15"/>
<connect gate="-7" pin="IO272" pad="A17"/>
<connect gate="-7" pin="IO273" pad="D15"/>
<connect gate="-7" pin="IO274" pad="Y15"/>
<connect gate="-7" pin="IO281" pad="U15"/>
<connect gate="-7" pin="IO282" pad="E15"/>
<connect gate="-7" pin="IO283" pad="F15"/>
<connect gate="-7" pin="IO284" pad="AA16"/>
<connect gate="-8" pin="IO291" pad="W15"/>
<connect gate="-8" pin="IO292" pad="F16"/>
<connect gate="-8" pin="IO293" pad="U17"/>
<connect gate="-8" pin="IO294" pad="A18"/>
<connect gate="-8" pin="IO301" pad="U16"/>
<connect gate="-8" pin="IO302" pad="D16"/>
<connect gate="-8" pin="IO303" pad="A19"/>
<connect gate="-8" pin="IO304" pad="AA17"/>
<connect gate="-8" pin="IO311" pad="W16"/>
<connect gate="-8" pin="IO312" pad="E16"/>
<connect gate="-8" pin="IO313" pad="AA18"/>
<connect gate="-8" pin="IO314" pad="B18"/>
<connect gate="-8" pin="IO321" pad="V16"/>
<connect gate="-8" pin="IO322" pad="G17"/>
<connect gate="-8" pin="IO323" pad="G16"/>
<connect gate="-8" pin="IO324" pad="Y17"/>
<connect gate="-9" pin="IO331" pad="V17"/>
<connect gate="-9" pin="IO332" pad="F17"/>
<connect gate="-9" pin="IO333" pad="Y18"/>
<connect gate="-9" pin="IO334" pad="C18"/>
<connect gate="-9" pin="IO341" pad="W17"/>
<connect gate="-9" pin="IO342" pad="D17"/>
<connect gate="-9" pin="IO343" pad="E17"/>
<connect gate="-9" pin="IO344" pad="AA19"/>
<connect gate="-9" pin="IO351" pad="W18"/>
<connect gate="-9" pin="IO352" pad="D18"/>
<connect gate="-9" pin="IO353" pad="AA20"/>
<connect gate="-9" pin="IO354" pad="C19"/>
<connect gate="-9" pin="IO361" pad="V18"/>
<connect gate="-9" pin="IO362" pad="D19"/>
<connect gate="-9" pin="IO363" pad="U19"/>
<connect gate="-9" pin="IO364" pad="C20"/>
<connect gate="-A" pin="IOA1" pad="H16"/>
<connect gate="-A" pin="IOA10" pad="G6"/>
<connect gate="-A" pin="IOA11" pad="J6"/>
<connect gate="-A" pin="IOA12" pad="J16"/>
<connect gate="-A" pin="IOA2" pad="H17"/>
<connect gate="-A" pin="IOA3" pad="G19"/>
<connect gate="-A" pin="IOA4" pad="G18"/>
<connect gate="-A" pin="IOA5" pad="H18"/>
<connect gate="-A" pin="IOA6" pad="H4"/>
<connect gate="-A" pin="IOA7" pad="J7"/>
<connect gate="-A" pin="IOA8" pad="G5"/>
<connect gate="-A" pin="IOA9" pad="F4"/>
<connect gate="-B" pin="IOB1" pad="J17"/>
<connect gate="-B" pin="IOB10" pad="H5"/>
<connect gate="-B" pin="IOB11" pad="J19"/>
<connect gate="-B" pin="IOB2" pad="K15"/>
<connect gate="-B" pin="IOB3" pad="K16"/>
<connect gate="-B" pin="IOB4" pad="J18"/>
<connect gate="-B" pin="IOB5" pad="L8"/>
<connect gate="-B" pin="IOB6" pad="K7"/>
<connect gate="-B" pin="IOB7" pad="J5"/>
<connect gate="-B" pin="IOB8" pad="J4"/>
<connect gate="-B" pin="IOB9" pad="K8"/>
<connect gate="-C" pin="IOC1" pad="K17"/>
<connect gate="-C" pin="IOC10" pad="K5"/>
<connect gate="-C" pin="IOC11" pad="K4"/>
<connect gate="-C" pin="IOC12" pad="L16"/>
<connect gate="-C" pin="IOC2" pad="L15"/>
<connect gate="-C" pin="IOC3" pad="K18"/>
<connect gate="-C" pin="IOC4" pad="K19"/>
<connect gate="-C" pin="IOC5" pad="L17"/>
<connect gate="-C" pin="IOC6" pad="M8"/>
<connect gate="-C" pin="IOC7" pad="L5"/>
<connect gate="-C" pin="IOC8" pad="L6"/>
<connect gate="-C" pin="IOC9" pad="L7"/>
<connect gate="-D" pin="IOD1" pad="L18"/>
<connect gate="-D" pin="IOD10" pad="M6"/>
<connect gate="-D" pin="IOD11" pad="M7"/>
<connect gate="-D" pin="IOD12" pad="N7"/>
<connect gate="-D" pin="IOD2" pad="M15"/>
<connect gate="-D" pin="IOD3" pad="M16"/>
<connect gate="-D" pin="IOD4" pad="M17"/>
<connect gate="-D" pin="IOD5" pad="M19"/>
<connect gate="-D" pin="IOD6" pad="M18"/>
<connect gate="-D" pin="IOD7" pad="N15"/>
<connect gate="-D" pin="IOD8" pad="N4"/>
<connect gate="-D" pin="IOD9" pad="M5"/>
<connect gate="-E" pin="IOE1" pad="N18"/>
<connect gate="-E" pin="IOE10" pad="N5"/>
<connect gate="-E" pin="IOE11" pad="P6"/>
<connect gate="-E" pin="IOE2" pad="N16"/>
<connect gate="-E" pin="IOE3" pad="P17"/>
<connect gate="-E" pin="IOE4" pad="P18"/>
<connect gate="-E" pin="IOE5" pad="P19"/>
<connect gate="-E" pin="IOE6" pad="P16"/>
<connect gate="-E" pin="IOE7" pad="R5"/>
<connect gate="-E" pin="IOE8" pad="P4"/>
<connect gate="-E" pin="IOE9" pad="N8"/>
<connect gate="-F" pin="IOF1" pad="R18"/>
<connect gate="-F" pin="IOF10" pad="R4"/>
<connect gate="-F" pin="IOF11" pad="R6"/>
<connect gate="-F" pin="IOF12" pad="T16"/>
<connect gate="-F" pin="IOF2" pad="R16"/>
<connect gate="-F" pin="IOF3" pad="T17"/>
<connect gate="-F" pin="IOF4" pad="T19"/>
<connect gate="-F" pin="IOF5" pad="U5"/>
<connect gate="-F" pin="IOF6" pad="T4"/>
<connect gate="-F" pin="IOF7" pad="T6"/>
<connect gate="-F" pin="IOF8" pad="T5"/>
<connect gate="-F" pin="IOF9" pad="R7"/>
<connect gate="G1" pin="GND" pad="AA1"/>
<connect gate="G10" pin="GND" pad="B2"/>
<connect gate="G11" pin="GND" pad="B17"/>
<connect gate="G12" pin="GND" pad="B21"/>
<connect gate="G13" pin="GND" pad="B22"/>
<connect gate="G14" pin="GND" pad="C2"/>
<connect gate="G15" pin="GND" pad="C21"/>
<connect gate="G16" pin="GND" pad="E21"/>
<connect gate="G17" pin="GND" pad="G3"/>
<connect gate="G18" pin="GND" pad="G21"/>
<connect gate="G19" pin="GND" pad="H2"/>
<connect gate="G2" pin="GND" pad="AA6"/>
<connect gate="G20" pin="GND" pad="H8"/>
<connect gate="G21" pin="GND" pad="H15"/>
<connect gate="G22" pin="GND" pad="J9"/>
<connect gate="G23" pin="GND" pad="J14"/>
<connect gate="G24" pin="GND" pad="J20"/>
<connect gate="G25" pin="GND" pad="K3"/>
<connect gate="G26" pin="GND" pad="K10"/>
<connect gate="G27" pin="GND" pad="K12"/>
<connect gate="G28" pin="GND" pad="K13"/>
<connect gate="G29" pin="GND" pad="L11"/>
<connect gate="G3" pin="GND" pad="AA22"/>
<connect gate="G30" pin="GND" pad="L12"/>
<connect gate="G31" pin="GND" pad="M11"/>
<connect gate="G32" pin="GND" pad="M12"/>
<connect gate="G33" pin="GND" pad="M20"/>
<connect gate="G34" pin="GND" pad="N10"/>
<connect gate="G35" pin="GND" pad="N13"/>
<connect gate="G36" pin="GND" pad="P9"/>
<connect gate="G37" pin="GND" pad="P14"/>
<connect gate="G38" pin="GND" pad="R8"/>
<connect gate="G39" pin="GND" pad="R15"/>
<connect gate="G4" pin="GND" pad="AB11"/>
<connect gate="G40" pin="GND" pad="R22"/>
<connect gate="G41" pin="GND" pad="T1"/>
<connect gate="G42" pin="GND" pad="V3"/>
<connect gate="G43" pin="GND" pad="W11"/>
<connect gate="G44" pin="GND" pad="W20"/>
<connect gate="G45" pin="GND" pad="Y1"/>
<connect gate="G46" pin="GND" pad="Y2"/>
<connect gate="G47" pin="GND" pad="Y3"/>
<connect gate="G48" pin="GND" pad="Y21"/>
<connect gate="G49" pin="GND" pad="Y22"/>
<connect gate="G5" pin="GND" pad="AB16"/>
<connect gate="G6" pin="GND" pad="A1"/>
<connect gate="G7" pin="GND" pad="A8"/>
<connect gate="G8" pin="GND" pad="A22"/>
<connect gate="G9" pin="GND" pad="B1"/>
<connect gate="NC1" pin="NC" pad="AA2"/>
<connect gate="NC10" pin="NC" pad="AB2"/>
<connect gate="NC100" pin="NC" pad="M2"/>
<connect gate="NC101" pin="NC" pad="M3"/>
<connect gate="NC102" pin="NC" pad="M4"/>
<connect gate="NC103" pin="NC" pad="M21"/>
<connect gate="NC104" pin="NC" pad="M22"/>
<connect gate="NC105" pin="NC" pad="N1"/>
<connect gate="NC106" pin="NC" pad="N2"/>
<connect gate="NC107" pin="NC" pad="N6"/>
<connect gate="NC108" pin="NC" pad="N17"/>
<connect gate="NC109" pin="NC" pad="N19"/>
<connect gate="NC11" pin="NC" pad="AB3"/>
<connect gate="NC110" pin="NC" pad="U21"/>
<connect gate="NC111" pin="NC" pad="N21"/>
<connect gate="NC112" pin="NC" pad="N22"/>
<connect gate="NC113" pin="NC" pad="P1"/>
<connect gate="NC114" pin="NC" pad="P2"/>
<connect gate="NC115" pin="NC" pad="P3"/>
<connect gate="NC116" pin="NC" pad="P5"/>
<connect gate="NC117" pin="NC" pad="P7"/>
<connect gate="NC118" pin="NC" pad="P20"/>
<connect gate="NC119" pin="NC" pad="P21"/>
<connect gate="NC12" pin="NC" pad="AB4"/>
<connect gate="NC120" pin="NC" pad="P22"/>
<connect gate="NC121" pin="NC" pad="R2"/>
<connect gate="NC122" pin="NC" pad="R3"/>
<connect gate="NC123" pin="NC" pad="R17"/>
<connect gate="NC124" pin="NC" pad="R19"/>
<connect gate="NC125" pin="NC" pad="R20"/>
<connect gate="NC126" pin="NC" pad="R21"/>
<connect gate="NC127" pin="NC" pad="T2"/>
<connect gate="NC128" pin="NC" pad="T18"/>
<connect gate="NC129" pin="NC" pad="T20"/>
<connect gate="NC13" pin="NC" pad="AB5"/>
<connect gate="NC130" pin="NC" pad="T21"/>
<connect gate="NC131" pin="NC" pad="U1"/>
<connect gate="NC132" pin="NC" pad="U2"/>
<connect gate="NC133" pin="NC" pad="U3"/>
<connect gate="NC134" pin="NC" pad="U20"/>
<connect gate="NC135" pin="NC" pad="U22"/>
<connect gate="NC136" pin="NC" pad="V1"/>
<connect gate="NC137" pin="NC" pad="V2"/>
<connect gate="NC138" pin="NC" pad="V20"/>
<connect gate="NC139" pin="NC" pad="V21"/>
<connect gate="NC14" pin="NC" pad="AB7"/>
<connect gate="NC140" pin="NC" pad="W1"/>
<connect gate="NC141" pin="NC" pad="W2"/>
<connect gate="NC142" pin="NC" pad="W22"/>
<connect gate="NC143" pin="NC" pad="Y4"/>
<connect gate="NC144" pin="NC" pad="Y9"/>
<connect gate="NC145" pin="NC" pad="Y12"/>
<connect gate="NC146" pin="NC" pad="Y13"/>
<connect gate="NC147" pin="NC" pad="Y16"/>
<connect gate="NC148" pin="NC" pad="Y19"/>
<connect gate="NC149" pin="NC" pad="Y20"/>
<connect gate="NC15" pin="NC" pad="AB8"/>
<connect gate="NC16" pin="NC" pad="AB9"/>
<connect gate="NC17" pin="NC" pad="AB12"/>
<connect gate="NC18" pin="NC" pad="AB15"/>
<connect gate="NC19" pin="NC" pad="AB17"/>
<connect gate="NC2" pin="NC" pad="AA3"/>
<connect gate="NC20" pin="NC" pad="AB18"/>
<connect gate="NC21" pin="NC" pad="AB19"/>
<connect gate="NC22" pin="NC" pad="AB20"/>
<connect gate="NC23" pin="NC" pad="AB21"/>
<connect gate="NC24" pin="NC" pad="AB22"/>
<connect gate="NC25" pin="NC" pad="A2"/>
<connect gate="NC26" pin="NC" pad="A3"/>
<connect gate="NC27" pin="NC" pad="A4"/>
<connect gate="NC28" pin="NC" pad="A5"/>
<connect gate="NC29" pin="NC" pad="A7"/>
<connect gate="NC3" pin="NC" pad="AA4"/>
<connect gate="NC30" pin="NC" pad="A9"/>
<connect gate="NC31" pin="NC" pad="A11"/>
<connect gate="NC32" pin="NC" pad="A12"/>
<connect gate="NC33" pin="NC" pad="A14"/>
<connect gate="NC34" pin="NC" pad="A15"/>
<connect gate="NC35" pin="NC" pad="A20"/>
<connect gate="NC36" pin="NC" pad="A21"/>
<connect gate="NC37" pin="NC" pad="B3"/>
<connect gate="NC38" pin="NC" pad="B4"/>
<connect gate="NC39" pin="NC" pad="B9"/>
<connect gate="NC4" pin="NC" pad="AA9"/>
<connect gate="NC40" pin="NC" pad="B10"/>
<connect gate="NC41" pin="NC" pad="B12"/>
<connect gate="NC42" pin="NC" pad="B16"/>
<connect gate="NC43" pin="NC" pad="B19"/>
<connect gate="NC44" pin="NC" pad="B20"/>
<connect gate="NC45" pin="NC" pad="C1"/>
<connect gate="NC46" pin="NC" pad="C6"/>
<connect gate="NC47" pin="NC" pad="C9"/>
<connect gate="NC48" pin="NC" pad="C10"/>
<connect gate="NC49" pin="NC" pad="C12"/>
<connect gate="NC5" pin="NC" pad="AA11"/>
<connect gate="NC50" pin="NC" pad="C13"/>
<connect gate="NC51" pin="NC" pad="C14"/>
<connect gate="NC52" pin="NC" pad="C16"/>
<connect gate="NC53" pin="NC" pad="C17"/>
<connect gate="NC54" pin="NC" pad="C22"/>
<connect gate="NC55" pin="NC" pad="D1"/>
<connect gate="NC56" pin="NC" pad="D2"/>
<connect gate="NC57" pin="NC" pad="D3"/>
<connect gate="NC58" pin="NC" pad="D20"/>
<connect gate="NC59" pin="NC" pad="D21"/>
<connect gate="NC6" pin="NC" pad="AA13"/>
<connect gate="NC60" pin="NC" pad="D22"/>
<connect gate="NC61" pin="NC" pad="E2"/>
<connect gate="NC62" pin="NC" pad="E3"/>
<connect gate="NC63" pin="NC" pad="E20"/>
<connect gate="NC64" pin="NC" pad="E22"/>
<connect gate="NC65" pin="NC" pad="F1"/>
<connect gate="NC66" pin="NC" pad="F2"/>
<connect gate="NC67" pin="NC" pad="F3"/>
<connect gate="NC68" pin="NC" pad="F20"/>
<connect gate="NC69" pin="NC" pad="F21"/>
<connect gate="NC7" pin="NC" pad="AA15"/>
<connect gate="NC70" pin="NC" pad="F22"/>
<connect gate="NC71" pin="NC" pad="G2"/>
<connect gate="NC72" pin="NC" pad="G4"/>
<connect gate="NC73" pin="NC" pad="G20"/>
<connect gate="NC74" pin="NC" pad="G22"/>
<connect gate="NC75" pin="NC" pad="H1"/>
<connect gate="NC76" pin="NC" pad="H3"/>
<connect gate="NC77" pin="NC" pad="H6"/>
<connect gate="NC78" pin="NC" pad="H19"/>
<connect gate="NC79" pin="NC" pad="H21"/>
<connect gate="NC8" pin="NC" pad="AA21"/>
<connect gate="NC80" pin="NC" pad="H22"/>
<connect gate="NC81" pin="NC" pad="J1"/>
<connect gate="NC82" pin="NC" pad="J2"/>
<connect gate="NC83" pin="NC" pad="J3"/>
<connect gate="NC84" pin="NC" pad="J21"/>
<connect gate="NC85" pin="NC" pad="J22"/>
<connect gate="NC86" pin="NC" pad="K1"/>
<connect gate="NC87" pin="NC" pad="K2"/>
<connect gate="NC88" pin="NC" pad="K6"/>
<connect gate="NC89" pin="NC" pad="K21"/>
<connect gate="NC9" pin="NC" pad="AB1"/>
<connect gate="NC90" pin="NC" pad="K22"/>
<connect gate="NC91" pin="NC" pad="L1"/>
<connect gate="NC92" pin="NC" pad="L2"/>
<connect gate="NC93" pin="NC" pad="L3"/>
<connect gate="NC94" pin="NC" pad="L4"/>
<connect gate="NC95" pin="NC" pad="L19"/>
<connect gate="NC96" pin="NC" pad="L20"/>
<connect gate="NC97" pin="NC" pad="L21"/>
<connect gate="NC98" pin="NC" pad="L22"/>
<connect gate="NC99" pin="NC" pad="M1"/>
<connect gate="V1" pin="VCC" pad="AA12"/>
<connect gate="V10" pin="VCC" pad="L10"/>
<connect gate="V11" pin="VCC" pad="L13"/>
<connect gate="V12" pin="VCC" pad="M10"/>
<connect gate="V13" pin="VCC" pad="M13"/>
<connect gate="V14" pin="VCC" pad="M14"/>
<connect gate="V15" pin="VCC" pad="N12"/>
<connect gate="V16" pin="VCC" pad="P8"/>
<connect gate="V17" pin="VCC" pad="P10"/>
<connect gate="V18" pin="VCC" pad="P12"/>
<connect gate="V19" pin="VCC" pad="P15"/>
<connect gate="V2" pin="VCC" pad="C11"/>
<connect gate="V20" pin="VCC" pad="R14"/>
<connect gate="V21" pin="VCC" pad="V5"/>
<connect gate="V22" pin="VCC" pad="W21"/>
<connect gate="V23" pin="VCC" pad="Y8"/>
<connect gate="V3" pin="VCC" pad="C15"/>
<connect gate="V4" pin="VCC" pad="H14"/>
<connect gate="V5" pin="VCC" pad="J8"/>
<connect gate="V6" pin="VCC" pad="J10"/>
<connect gate="V7" pin="VCC" pad="J12"/>
<connect gate="V8" pin="VCC" pad="J15"/>
<connect gate="V9" pin="VCC" pad="L9"/>
<connect gate="VO1" pin="VCCIO" pad="AB13"/>
<connect gate="VO10" pin="VCCIO" pad="J11"/>
<connect gate="VO11" pin="VCCIO" pad="J13"/>
<connect gate="VO12" pin="VCCIO" pad="K9"/>
<connect gate="VO13" pin="VCCIO" pad="K11"/>
<connect gate="VO14" pin="VCCIO" pad="K14"/>
<connect gate="VO15" pin="VCCIO" pad="K20"/>
<connect gate="VO16" pin="VCCIO" pad="L14"/>
<connect gate="VO17" pin="VCCIO" pad="M9"/>
<connect gate="VO18" pin="VCCIO" pad="N3"/>
<connect gate="VO19" pin="VCCIO" pad="N9"/>
<connect gate="VO2" pin="VCCIO" pad="A6"/>
<connect gate="VO20" pin="VCCIO" pad="N11"/>
<connect gate="VO21" pin="VCCIO" pad="N14"/>
<connect gate="VO22" pin="VCCIO" pad="N20"/>
<connect gate="VO23" pin="VCCIO" pad="P13"/>
<connect gate="VO24" pin="VCCIO" pad="R1"/>
<connect gate="VO25" pin="VCCIO" pad="R9"/>
<connect gate="VO26" pin="VCCIO" pad="T3"/>
<connect gate="VO27" pin="VCCIO" pad="T15"/>
<connect gate="VO28" pin="VCCIO" pad="T22"/>
<connect gate="VO29" pin="VCCIO" pad="V22"/>
<connect gate="VO3" pin="VCCIO" pad="A13"/>
<connect gate="VO4" pin="VCCIO" pad="B5"/>
<connect gate="VO5" pin="VCCIO" pad="E1"/>
<connect gate="VO6" pin="VCCIO" pad="G1"/>
<connect gate="VO7" pin="VCCIO" pad="G15"/>
<connect gate="VO8" pin="VCCIO" pad="H9"/>
<connect gate="VO9" pin="VCCIO" pad="H20"/>
<connect gate="_" pin="/CE" pad="E4"/>
<connect gate="_" pin="/CEO" pad="E19"/>
<connect gate="_" pin="/CONFIG" pad="T7"/>
<connect gate="_" pin="/STATUS" pad="W19"/>
<connect gate="_" pin="CONF_DONE" pad="F18"/>
<connect gate="_" pin="DATA0" pad="D4"/>
<connect gate="_" pin="DCLK" pad="E5"/>
<connect gate="_" pin="GCLK0" pad="P11"/>
<connect gate="_" pin="GCLK1" pad="D12"/>
<connect gate="_" pin="IN0" pad="R12"/>
<connect gate="_" pin="IN1" pad="V11"/>
<connect gate="_" pin="IN2" pad="H11"/>
<connect gate="_" pin="IN3" pad="E12"/>
<connect gate="_" pin="MSEL0" pad="U4"/>
<connect gate="_" pin="MSEL1" pad="V4"/>
<connect gate="_" pin="TCK" pad="E18"/>
<connect gate="_" pin="TDI" pad="F5"/>
<connect gate="_" pin="TDO" pad="F19"/>
<connect gate="_" pin="TMS" pad="U18"/>
<connect gate="_" pin="TRST" pad="V19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30AFC484-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8942"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30-FBGA484" prefix="IC">
<description>&lt;b&gt;EPF10K30A&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A16"/>
<gate name="-B" symbol="B16"/>
<gate name="-C" symbol="C16"/>
<gate name="-D" symbol="D16"/>
<gate name="-E" symbol="E16"/>
<gate name="-F" symbol="F16"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="G19" symbol="GND"/>
<gate name="G20" symbol="GND"/>
<gate name="G21" symbol="GND"/>
<gate name="G22" symbol="GND"/>
<gate name="G23" symbol="GND"/>
<gate name="G24" symbol="GND"/>
<gate name="G25" symbol="GND"/>
<gate name="G26" symbol="GND"/>
<gate name="G27" symbol="GND"/>
<gate name="G28" symbol="GND"/>
<gate name="G29" symbol="GND"/>
<gate name="G30" symbol="GND"/>
<gate name="G31" symbol="GND"/>
<gate name="G32" symbol="GND"/>
<gate name="G33" symbol="GND"/>
<gate name="G34" symbol="GND"/>
<gate name="G35" symbol="GND"/>
<gate name="G36" symbol="GND"/>
<gate name="G37" symbol="GND"/>
<gate name="G38" symbol="GND"/>
<gate name="G39" symbol="GND"/>
<gate name="G40" symbol="GND"/>
<gate name="G41" symbol="GND"/>
<gate name="G42" symbol="GND"/>
<gate name="G43" symbol="GND"/>
<gate name="G44" symbol="GND"/>
<gate name="G45" symbol="GND"/>
<gate name="G46" symbol="GND"/>
<gate name="G47" symbol="GND"/>
<gate name="G48" symbol="GND"/>
<gate name="G49" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="NC29" symbol="NC"/>
<gate name="NC30" symbol="NC"/>
<gate name="NC31" symbol="NC"/>
<gate name="NC32" symbol="NC"/>
<gate name="NC33" symbol="NC"/>
<gate name="NC34" symbol="NC"/>
<gate name="NC35" symbol="NC"/>
<gate name="NC36" symbol="NC"/>
<gate name="NC37" symbol="NC"/>
<gate name="NC38" symbol="NC"/>
<gate name="NC39" symbol="NC"/>
<gate name="NC40" symbol="NC"/>
<gate name="NC41" symbol="NC"/>
<gate name="NC42" symbol="NC"/>
<gate name="NC43" symbol="NC"/>
<gate name="NC44" symbol="NC"/>
<gate name="NC45" symbol="NC"/>
<gate name="NC46" symbol="NC"/>
<gate name="NC47" symbol="NC"/>
<gate name="NC48" symbol="NC"/>
<gate name="NC49" symbol="NC"/>
<gate name="NC50" symbol="NC"/>
<gate name="NC51" symbol="NC"/>
<gate name="NC52" symbol="NC"/>
<gate name="NC53" symbol="NC"/>
<gate name="NC54" symbol="NC"/>
<gate name="NC55" symbol="NC"/>
<gate name="NC56" symbol="NC"/>
<gate name="NC57" symbol="NC"/>
<gate name="NC58" symbol="NC"/>
<gate name="NC59" symbol="NC"/>
<gate name="NC60" symbol="NC"/>
<gate name="NC61" symbol="NC"/>
<gate name="NC62" symbol="NC"/>
<gate name="NC63" symbol="NC"/>
<gate name="NC64" symbol="NC"/>
<gate name="NC65" symbol="NC"/>
<gate name="NC66" symbol="NC"/>
<gate name="NC67" symbol="NC"/>
<gate name="NC68" symbol="NC"/>
<gate name="NC69" symbol="NC"/>
<gate name="NC70" symbol="NC"/>
<gate name="NC71" symbol="NC"/>
<gate name="NC72" symbol="NC"/>
<gate name="NC73" symbol="NC"/>
<gate name="NC74" symbol="NC"/>
<gate name="NC75" symbol="NC"/>
<gate name="NC76" symbol="NC"/>
<gate name="NC77" symbol="NC"/>
<gate name="NC78" symbol="NC"/>
<gate name="NC79" symbol="NC"/>
<gate name="NC80" symbol="NC"/>
<gate name="NC81" symbol="NC"/>
<gate name="NC82" symbol="NC"/>
<gate name="NC83" symbol="NC"/>
<gate name="NC84" symbol="NC"/>
<gate name="NC85" symbol="NC"/>
<gate name="NC86" symbol="NC"/>
<gate name="NC87" symbol="NC"/>
<gate name="NC88" symbol="NC"/>
<gate name="NC89" symbol="NC"/>
<gate name="NC90" symbol="NC"/>
<gate name="NC91" symbol="NC"/>
<gate name="NC92" symbol="NC"/>
<gate name="NC93" symbol="NC"/>
<gate name="NC94" symbol="NC"/>
<gate name="NC95" symbol="NC"/>
<gate name="NC96" symbol="NC"/>
<gate name="NC97" symbol="NC"/>
<gate name="NC98" symbol="NC"/>
<gate name="NC99" symbol="NC"/>
<gate name="NC100" symbol="NC"/>
<gate name="NC101" symbol="NC"/>
<gate name="NC102" symbol="NC"/>
<gate name="NC103" symbol="NC"/>
<gate name="NC104" symbol="NC"/>
<gate name="NC105" symbol="NC"/>
<gate name="NC106" symbol="NC"/>
<gate name="NC107" symbol="NC"/>
<gate name="NC108" symbol="NC"/>
<gate name="NC109" symbol="NC"/>
<gate name="NC110" symbol="NC"/>
<gate name="NC111" symbol="NC"/>
<gate name="NC112" symbol="NC"/>
<gate name="NC113" symbol="NC"/>
<gate name="NC114" symbol="NC"/>
<gate name="NC115" symbol="NC"/>
<gate name="NC116" symbol="NC"/>
<gate name="NC117" symbol="NC"/>
<gate name="NC118" symbol="NC"/>
<gate name="NC119" symbol="NC"/>
<gate name="NC120" symbol="NC"/>
<gate name="NC121" symbol="NC"/>
<gate name="NC122" symbol="NC"/>
<gate name="NC123" symbol="NC"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="V19" symbol="VCCINT"/>
<gate name="V20" symbol="VCCINT"/>
<gate name="V21" symbol="VCCINT"/>
<gate name="V22" symbol="VCCINT"/>
<gate name="V23" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
<gate name="VO20" symbol="VCCIO"/>
<gate name="VO21" symbol="VCCIO"/>
<gate name="VO22" symbol="VCCIO"/>
<gate name="VO23" symbol="VCCIO"/>
<gate name="VO24" symbol="VCCIO"/>
<gate name="VO25" symbol="VCCIO"/>
<gate name="VO26" symbol="VCCIO"/>
<gate name="VO27" symbol="VCCIO"/>
<gate name="VO28" symbol="VCCIO"/>
<gate name="VO29" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="FBGA484">
<connects>
<connect gate="-1" pin="IO11" pad="W4"/>
<connect gate="-1" pin="IO12" pad="E6"/>
<connect gate="-1" pin="IO13" pad="C3"/>
<connect gate="-1" pin="IO14" pad="W3"/>
<connect gate="-1" pin="IO21" pad="W6"/>
<connect gate="-1" pin="IO22" pad="W5"/>
<connect gate="-1" pin="IO23" pad="D5"/>
<connect gate="-1" pin="IO24" pad="C4"/>
<connect gate="-1" pin="IO31" pad="U6"/>
<connect gate="-1" pin="IO32" pad="F6"/>
<connect gate="-1" pin="IO33" pad="C5"/>
<connect gate="-1" pin="IO34" pad="Y5"/>
<connect gate="-1" pin="IO41" pad="V6"/>
<connect gate="-1" pin="IO42" pad="D6"/>
<connect gate="-1" pin="IO43" pad="E7"/>
<connect gate="-1" pin="IO44" pad="AA5"/>
<connect gate="-2" pin="IO51" pad="Y6"/>
<connect gate="-2" pin="IO52" pad="U7"/>
<connect gate="-2" pin="IO53" pad="D7"/>
<connect gate="-2" pin="IO54" pad="B6"/>
<connect gate="-2" pin="IO61" pad="W7"/>
<connect gate="-2" pin="IO62" pad="F7"/>
<connect gate="-2" pin="IO63" pad="G7"/>
<connect gate="-2" pin="IO64" pad="Y7"/>
<connect gate="-2" pin="IO71" pad="T8"/>
<connect gate="-2" pin="IO72" pad="V7"/>
<connect gate="-2" pin="IO73" pad="E8"/>
<connect gate="-2" pin="IO74" pad="C7"/>
<connect gate="-2" pin="IO81" pad="U8"/>
<connect gate="-2" pin="IO82" pad="B7"/>
<connect gate="-2" pin="IO83" pad="D8"/>
<connect gate="-2" pin="IO84" pad="AB6"/>
<connect gate="-3" pin="IO101" pad="T9"/>
<connect gate="-3" pin="IO102" pad="G8"/>
<connect gate="-3" pin="IO103" pad="B8"/>
<connect gate="-3" pin="IO104" pad="V8"/>
<connect gate="-3" pin="IO111" pad="U9"/>
<connect gate="-3" pin="IO112" pad="H7"/>
<connect gate="-3" pin="IO113" pad="E9"/>
<connect gate="-3" pin="IO114" pad="AA8"/>
<connect gate="-3" pin="IO121" pad="V9"/>
<connect gate="-3" pin="IO122" pad="W9"/>
<connect gate="-3" pin="IO123" pad="F9"/>
<connect gate="-3" pin="IO124" pad="D9"/>
<connect gate="-3" pin="IO91" pad="W8"/>
<connect gate="-3" pin="IO92" pad="AA7"/>
<connect gate="-3" pin="IO93" pad="F8"/>
<connect gate="-3" pin="IO94" pad="C8"/>
<connect gate="-4" pin="IO131" pad="T10"/>
<connect gate="-4" pin="IO132" pad="R10"/>
<connect gate="-4" pin="IO133" pad="G9"/>
<connect gate="-4" pin="IO134" pad="A10"/>
<connect gate="-4" pin="IO141" pad="W10"/>
<connect gate="-4" pin="IO142" pad="D10"/>
<connect gate="-4" pin="IO143" pad="E10"/>
<connect gate="-4" pin="IO144" pad="U10"/>
<connect gate="-4" pin="IO151" pad="V10"/>
<connect gate="-4" pin="IO152" pad="F10"/>
<connect gate="-4" pin="IO153" pad="G10"/>
<connect gate="-4" pin="IO154" pad="Y10"/>
<connect gate="-4" pin="IO161" pad="R11"/>
<connect gate="-4" pin="IO162" pad="H10"/>
<connect gate="-4" pin="IO163" pad="AA10"/>
<connect gate="-4" pin="IO164" pad="B11"/>
<connect gate="-5" pin="IO171" pad="T11"/>
<connect gate="-5" pin="IO172" pad="D11"/>
<connect gate="-5" pin="IO173" pad="E11"/>
<connect gate="-5" pin="IO174" pad="AB10"/>
<connect gate="-5" pin="IO181" pad="U11"/>
<connect gate="-5" pin="IO182" pad="F11"/>
<connect gate="-5" pin="IO183" pad="G11"/>
<connect gate="-5" pin="IO184" pad="Y11"/>
<connect gate="-5" pin="IO191" pad="W12"/>
<connect gate="-5" pin="IO192" pad="V12"/>
<connect gate="-5" pin="IO193" pad="F12"/>
<connect gate="-5" pin="IO194" pad="B13"/>
<connect gate="-5" pin="IO201" pad="T12"/>
<connect gate="-5" pin="IO202" pad="G12"/>
<connect gate="-5" pin="IO203" pad="H12"/>
<connect gate="-5" pin="IO204" pad="U12"/>
<connect gate="-6" pin="IO211" pad="V13"/>
<connect gate="-6" pin="IO212" pad="U13"/>
<connect gate="-6" pin="IO213" pad="D13"/>
<connect gate="-6" pin="IO214" pad="B14"/>
<connect gate="-6" pin="IO221" pad="W13"/>
<connect gate="-6" pin="IO222" pad="E13"/>
<connect gate="-6" pin="IO223" pad="F13"/>
<connect gate="-6" pin="IO224" pad="AB14"/>
<connect gate="-6" pin="IO231" pad="T13"/>
<connect gate="-6" pin="IO232" pad="G13"/>
<connect gate="-6" pin="IO233" pad="H13"/>
<connect gate="-6" pin="IO234" pad="AA14"/>
<connect gate="-6" pin="IO241" pad="R13"/>
<connect gate="-6" pin="IO242" pad="D14"/>
<connect gate="-6" pin="IO243" pad="B15"/>
<connect gate="-6" pin="IO244" pad="Y14"/>
<connect gate="-7" pin="IO251" pad="W14"/>
<connect gate="-7" pin="IO252" pad="V14"/>
<connect gate="-7" pin="IO253" pad="E14"/>
<connect gate="-7" pin="IO254" pad="A16"/>
<connect gate="-7" pin="IO261" pad="T14"/>
<connect gate="-7" pin="IO262" pad="U14"/>
<connect gate="-7" pin="IO263" pad="G14"/>
<connect gate="-7" pin="IO264" pad="F14"/>
<connect gate="-7" pin="IO271" pad="V15"/>
<connect gate="-7" pin="IO272" pad="D15"/>
<connect gate="-7" pin="IO273" pad="A17"/>
<connect gate="-7" pin="IO274" pad="Y15"/>
<connect gate="-7" pin="IO281" pad="U15"/>
<connect gate="-7" pin="IO282" pad="F15"/>
<connect gate="-7" pin="IO283" pad="AA16"/>
<connect gate="-7" pin="IO284" pad="E15"/>
<connect gate="-8" pin="IO291" pad="U17"/>
<connect gate="-8" pin="IO292" pad="W15"/>
<connect gate="-8" pin="IO293" pad="F16"/>
<connect gate="-8" pin="IO294" pad="A18"/>
<connect gate="-8" pin="IO301" pad="U16"/>
<connect gate="-8" pin="IO302" pad="A19"/>
<connect gate="-8" pin="IO303" pad="D16"/>
<connect gate="-8" pin="IO304" pad="AA17"/>
<connect gate="-8" pin="IO311" pad="W16"/>
<connect gate="-8" pin="IO312" pad="AA18"/>
<connect gate="-8" pin="IO313" pad="E16"/>
<connect gate="-8" pin="IO314" pad="B18"/>
<connect gate="-8" pin="IO321" pad="V16"/>
<connect gate="-8" pin="IO322" pad="G16"/>
<connect gate="-8" pin="IO323" pad="G17"/>
<connect gate="-8" pin="IO324" pad="Y17"/>
<connect gate="-9" pin="IO331" pad="V17"/>
<connect gate="-9" pin="IO332" pad="F17"/>
<connect gate="-9" pin="IO333" pad="C18"/>
<connect gate="-9" pin="IO334" pad="Y18"/>
<connect gate="-9" pin="IO341" pad="W17"/>
<connect gate="-9" pin="IO342" pad="D17"/>
<connect gate="-9" pin="IO343" pad="E17"/>
<connect gate="-9" pin="IO344" pad="AA19"/>
<connect gate="-9" pin="IO351" pad="W18"/>
<connect gate="-9" pin="IO352" pad="D18"/>
<connect gate="-9" pin="IO353" pad="AA20"/>
<connect gate="-9" pin="IO354" pad="C19"/>
<connect gate="-9" pin="IO361" pad="V18"/>
<connect gate="-9" pin="IO362" pad="U19"/>
<connect gate="-9" pin="IO363" pad="D19"/>
<connect gate="-9" pin="IO364" pad="C20"/>
<connect gate="-A" pin="IOA1" pad="H16"/>
<connect gate="-A" pin="IOA10" pad="H6"/>
<connect gate="-A" pin="IOA11" pad="G6"/>
<connect gate="-A" pin="IOA12" pad="G5"/>
<connect gate="-A" pin="IOA13" pad="F4"/>
<connect gate="-A" pin="IOA14" pad="F22"/>
<connect gate="-A" pin="IOA15" pad="G4"/>
<connect gate="-A" pin="IOA16" pad="J6"/>
<connect gate="-A" pin="IOA2" pad="D22"/>
<connect gate="-A" pin="IOA3" pad="H17"/>
<connect gate="-A" pin="IOA4" pad="G19"/>
<connect gate="-A" pin="IOA5" pad="G18"/>
<connect gate="-A" pin="IOA6" pad="J16"/>
<connect gate="-A" pin="IOA7" pad="H18"/>
<connect gate="-A" pin="IOA8" pad="H4"/>
<connect gate="-A" pin="IOA9" pad="J7"/>
<connect gate="-B" pin="IOB1" pad="H19"/>
<connect gate="-B" pin="IOB10" pad="J5"/>
<connect gate="-B" pin="IOB11" pad="J4"/>
<connect gate="-B" pin="IOB12" pad="K8"/>
<connect gate="-B" pin="IOB13" pad="H1"/>
<connect gate="-B" pin="IOB14" pad="H5"/>
<connect gate="-B" pin="IOB15" pad="H22"/>
<connect gate="-B" pin="IOB16" pad="K6"/>
<connect gate="-B" pin="IOB2" pad="J17"/>
<connect gate="-B" pin="IOB3" pad="K15"/>
<connect gate="-B" pin="IOB4" pad="H21"/>
<connect gate="-B" pin="IOB5" pad="K16"/>
<connect gate="-B" pin="IOB6" pad="J19"/>
<connect gate="-B" pin="IOB7" pad="J18"/>
<connect gate="-B" pin="IOB8" pad="L8"/>
<connect gate="-B" pin="IOB9" pad="K7"/>
<connect gate="-C" pin="IOC1" pad="K17"/>
<connect gate="-C" pin="IOC10" pad="L6"/>
<connect gate="-C" pin="IOC11" pad="L7"/>
<connect gate="-C" pin="IOC12" pad="K5"/>
<connect gate="-C" pin="IOC13" pad="K1"/>
<connect gate="-C" pin="IOC14" pad="K4"/>
<connect gate="-C" pin="IOC15" pad="L4"/>
<connect gate="-C" pin="IOC16" pad="L19"/>
<connect gate="-C" pin="IOC2" pad="L15"/>
<connect gate="-C" pin="IOC3" pad="K18"/>
<connect gate="-C" pin="IOC4" pad="K19"/>
<connect gate="-C" pin="IOC5" pad="K21"/>
<connect gate="-C" pin="IOC6" pad="L16"/>
<connect gate="-C" pin="IOC7" pad="L17"/>
<connect gate="-C" pin="IOC8" pad="M8"/>
<connect gate="-C" pin="IOC9" pad="L5"/>
<connect gate="-D" pin="IOD1" pad="L18"/>
<connect gate="-D" pin="IOD10" pad="M5"/>
<connect gate="-D" pin="IOD11" pad="M4"/>
<connect gate="-D" pin="IOD12" pad="M6"/>
<connect gate="-D" pin="IOD13" pad="M1"/>
<connect gate="-D" pin="IOD14" pad="M7"/>
<connect gate="-D" pin="IOD15" pad="N6"/>
<connect gate="-D" pin="IOD16" pad="N19"/>
<connect gate="-D" pin="IOD2" pad="M15"/>
<connect gate="-D" pin="IOD3" pad="M16"/>
<connect gate="-D" pin="IOD4" pad="M17"/>
<connect gate="-D" pin="IOD5" pad="M19"/>
<connect gate="-D" pin="IOD6" pad="M18"/>
<connect gate="-D" pin="IOD7" pad="N15"/>
<connect gate="-D" pin="IOD8" pad="N4"/>
<connect gate="-D" pin="IOD9" pad="N7"/>
<connect gate="-E" pin="IOE1" pad="N18"/>
<connect gate="-E" pin="IOE10" pad="P4"/>
<connect gate="-E" pin="IOE11" pad="P6"/>
<connect gate="-E" pin="IOE12" pad="N8"/>
<connect gate="-E" pin="IOE13" pad="P1"/>
<connect gate="-E" pin="IOE14" pad="N5"/>
<connect gate="-E" pin="IOE15" pad="P7"/>
<connect gate="-E" pin="IOE16" pad="R17"/>
<connect gate="-E" pin="IOE2" pad="N17"/>
<connect gate="-E" pin="IOE3" pad="N16"/>
<connect gate="-E" pin="IOE4" pad="P17"/>
<connect gate="-E" pin="IOE5" pad="P18"/>
<connect gate="-E" pin="IOE6" pad="P19"/>
<connect gate="-E" pin="IOE7" pad="P16"/>
<connect gate="-E" pin="IOE8" pad="R5"/>
<connect gate="-E" pin="IOE9" pad="P5"/>
<connect gate="-F" pin="IOF1" pad="R18"/>
<connect gate="-F" pin="IOF10" pad="T6"/>
<connect gate="-F" pin="IOF11" pad="T5"/>
<connect gate="-F" pin="IOF12" pad="R7"/>
<connect gate="-F" pin="IOF13" pad="R6"/>
<connect gate="-F" pin="IOF14" pad="R4"/>
<connect gate="-F" pin="IOF15" pad="V1"/>
<connect gate="-F" pin="IOF16" pad="V21"/>
<connect gate="-F" pin="IOF2" pad="R19"/>
<connect gate="-F" pin="IOF3" pad="R16"/>
<connect gate="-F" pin="IOF4" pad="T16"/>
<connect gate="-F" pin="IOF5" pad="T17"/>
<connect gate="-F" pin="IOF6" pad="T18"/>
<connect gate="-F" pin="IOF7" pad="T19"/>
<connect gate="-F" pin="IOF8" pad="U5"/>
<connect gate="-F" pin="IOF9" pad="T4"/>
<connect gate="G1" pin="GND" pad="AA1"/>
<connect gate="G10" pin="GND" pad="B2"/>
<connect gate="G11" pin="GND" pad="B17"/>
<connect gate="G12" pin="GND" pad="B21"/>
<connect gate="G13" pin="GND" pad="B22"/>
<connect gate="G14" pin="GND" pad="C2"/>
<connect gate="G15" pin="GND" pad="C21"/>
<connect gate="G16" pin="GND" pad="E21"/>
<connect gate="G17" pin="GND" pad="G3"/>
<connect gate="G18" pin="GND" pad="G21"/>
<connect gate="G19" pin="GND" pad="H2"/>
<connect gate="G2" pin="GND" pad="AA6"/>
<connect gate="G20" pin="GND" pad="H8"/>
<connect gate="G21" pin="GND" pad="H15"/>
<connect gate="G22" pin="GND" pad="J9"/>
<connect gate="G23" pin="GND" pad="J14"/>
<connect gate="G24" pin="GND" pad="J20"/>
<connect gate="G25" pin="GND" pad="K3"/>
<connect gate="G26" pin="GND" pad="K10"/>
<connect gate="G27" pin="GND" pad="K12"/>
<connect gate="G28" pin="GND" pad="K13"/>
<connect gate="G29" pin="GND" pad="L11"/>
<connect gate="G3" pin="GND" pad="AA22"/>
<connect gate="G30" pin="GND" pad="L12"/>
<connect gate="G31" pin="GND" pad="M11"/>
<connect gate="G32" pin="GND" pad="M12"/>
<connect gate="G33" pin="GND" pad="M20"/>
<connect gate="G34" pin="GND" pad="N10"/>
<connect gate="G35" pin="GND" pad="N13"/>
<connect gate="G36" pin="GND" pad="P9"/>
<connect gate="G37" pin="GND" pad="P14"/>
<connect gate="G38" pin="GND" pad="R8"/>
<connect gate="G39" pin="GND" pad="R15"/>
<connect gate="G4" pin="GND" pad="AB11"/>
<connect gate="G40" pin="GND" pad="R22"/>
<connect gate="G41" pin="GND" pad="T1"/>
<connect gate="G42" pin="GND" pad="V3"/>
<connect gate="G43" pin="GND" pad="W11"/>
<connect gate="G44" pin="GND" pad="W20"/>
<connect gate="G45" pin="GND" pad="Y1"/>
<connect gate="G46" pin="GND" pad="Y2"/>
<connect gate="G47" pin="GND" pad="Y3"/>
<connect gate="G48" pin="GND" pad="Y21"/>
<connect gate="G49" pin="GND" pad="Y22"/>
<connect gate="G5" pin="GND" pad="AB16"/>
<connect gate="G6" pin="GND" pad="A1"/>
<connect gate="G7" pin="GND" pad="A8"/>
<connect gate="G8" pin="GND" pad="A22"/>
<connect gate="G9" pin="GND" pad="B1"/>
<connect gate="NC1" pin="NC" pad="AA2"/>
<connect gate="NC10" pin="NC" pad="AB2"/>
<connect gate="NC100" pin="NC" pad="R3"/>
<connect gate="NC101" pin="NC" pad="R20"/>
<connect gate="NC102" pin="NC" pad="R21"/>
<connect gate="NC103" pin="NC" pad="T2"/>
<connect gate="NC104" pin="NC" pad="T20"/>
<connect gate="NC105" pin="NC" pad="T21"/>
<connect gate="NC106" pin="NC" pad="U1"/>
<connect gate="NC107" pin="NC" pad="U2"/>
<connect gate="NC108" pin="NC" pad="U3"/>
<connect gate="NC109" pin="NC" pad="U20"/>
<connect gate="NC11" pin="NC" pad="AB3"/>
<connect gate="NC110" pin="NC" pad="U21"/>
<connect gate="NC111" pin="NC" pad="U22"/>
<connect gate="NC112" pin="NC" pad="V2"/>
<connect gate="NC113" pin="NC" pad="V20"/>
<connect gate="NC114" pin="NC" pad="W1"/>
<connect gate="NC115" pin="NC" pad="W2"/>
<connect gate="NC116" pin="NC" pad="W22"/>
<connect gate="NC117" pin="NC" pad="Y4"/>
<connect gate="NC118" pin="NC" pad="Y9"/>
<connect gate="NC119" pin="NC" pad="Y12"/>
<connect gate="NC12" pin="NC" pad="AB4"/>
<connect gate="NC120" pin="NC" pad="Y13"/>
<connect gate="NC121" pin="NC" pad="Y16"/>
<connect gate="NC122" pin="NC" pad="Y19"/>
<connect gate="NC123" pin="NC" pad="Y20"/>
<connect gate="NC13" pin="NC" pad="AB5"/>
<connect gate="NC14" pin="NC" pad="AB7"/>
<connect gate="NC15" pin="NC" pad="AB8"/>
<connect gate="NC16" pin="NC" pad="AB9"/>
<connect gate="NC17" pin="NC" pad="AB12"/>
<connect gate="NC18" pin="NC" pad="AB15"/>
<connect gate="NC19" pin="NC" pad="AB17"/>
<connect gate="NC2" pin="NC" pad="AA3"/>
<connect gate="NC20" pin="NC" pad="AB18"/>
<connect gate="NC21" pin="NC" pad="AB19"/>
<connect gate="NC22" pin="NC" pad="AB20"/>
<connect gate="NC23" pin="NC" pad="AB21"/>
<connect gate="NC24" pin="NC" pad="AB22"/>
<connect gate="NC25" pin="NC" pad="A2"/>
<connect gate="NC26" pin="NC" pad="A3"/>
<connect gate="NC27" pin="NC" pad="A4"/>
<connect gate="NC28" pin="NC" pad="A5"/>
<connect gate="NC29" pin="NC" pad="A7"/>
<connect gate="NC3" pin="NC" pad="AA4"/>
<connect gate="NC30" pin="NC" pad="A9"/>
<connect gate="NC31" pin="NC" pad="A11"/>
<connect gate="NC32" pin="NC" pad="A12"/>
<connect gate="NC33" pin="NC" pad="A14"/>
<connect gate="NC34" pin="NC" pad="A15"/>
<connect gate="NC35" pin="NC" pad="A20"/>
<connect gate="NC36" pin="NC" pad="A21"/>
<connect gate="NC37" pin="NC" pad="B3"/>
<connect gate="NC38" pin="NC" pad="B4"/>
<connect gate="NC39" pin="NC" pad="B9"/>
<connect gate="NC4" pin="NC" pad="AA9"/>
<connect gate="NC40" pin="NC" pad="B10"/>
<connect gate="NC41" pin="NC" pad="B12"/>
<connect gate="NC42" pin="NC" pad="B16"/>
<connect gate="NC43" pin="NC" pad="B19"/>
<connect gate="NC44" pin="NC" pad="B20"/>
<connect gate="NC45" pin="NC" pad="C1"/>
<connect gate="NC46" pin="NC" pad="C6"/>
<connect gate="NC47" pin="NC" pad="C9"/>
<connect gate="NC48" pin="NC" pad="C10"/>
<connect gate="NC49" pin="NC" pad="C12"/>
<connect gate="NC5" pin="NC" pad="AA11"/>
<connect gate="NC50" pin="NC" pad="C13"/>
<connect gate="NC51" pin="NC" pad="C14"/>
<connect gate="NC52" pin="NC" pad="C16"/>
<connect gate="NC53" pin="NC" pad="C17"/>
<connect gate="NC54" pin="NC" pad="C22"/>
<connect gate="NC55" pin="NC" pad="D1"/>
<connect gate="NC56" pin="NC" pad="D2"/>
<connect gate="NC57" pin="NC" pad="D3"/>
<connect gate="NC58" pin="NC" pad="D20"/>
<connect gate="NC59" pin="NC" pad="D21"/>
<connect gate="NC6" pin="NC" pad="AA13"/>
<connect gate="NC60" pin="NC" pad="E2"/>
<connect gate="NC61" pin="NC" pad="E3"/>
<connect gate="NC62" pin="NC" pad="E20"/>
<connect gate="NC63" pin="NC" pad="E22"/>
<connect gate="NC64" pin="NC" pad="F1"/>
<connect gate="NC65" pin="NC" pad="F2"/>
<connect gate="NC66" pin="NC" pad="F3"/>
<connect gate="NC67" pin="NC" pad="F20"/>
<connect gate="NC68" pin="NC" pad="F21"/>
<connect gate="NC69" pin="NC" pad="G2"/>
<connect gate="NC7" pin="NC" pad="AA15"/>
<connect gate="NC70" pin="NC" pad="G20"/>
<connect gate="NC71" pin="NC" pad="G22"/>
<connect gate="NC72" pin="NC" pad="H3"/>
<connect gate="NC73" pin="NC" pad="J1"/>
<connect gate="NC74" pin="NC" pad="J2"/>
<connect gate="NC75" pin="NC" pad="J3"/>
<connect gate="NC76" pin="NC" pad="J21"/>
<connect gate="NC77" pin="NC" pad="J22"/>
<connect gate="NC78" pin="NC" pad="K2"/>
<connect gate="NC79" pin="NC" pad="K22"/>
<connect gate="NC8" pin="NC" pad="AA21"/>
<connect gate="NC80" pin="NC" pad="L1"/>
<connect gate="NC81" pin="NC" pad="L2"/>
<connect gate="NC82" pin="NC" pad="L3"/>
<connect gate="NC83" pin="NC" pad="L20"/>
<connect gate="NC84" pin="NC" pad="L21"/>
<connect gate="NC85" pin="NC" pad="L22"/>
<connect gate="NC86" pin="NC" pad="M2"/>
<connect gate="NC87" pin="NC" pad="M3"/>
<connect gate="NC88" pin="NC" pad="M21"/>
<connect gate="NC89" pin="NC" pad="M22"/>
<connect gate="NC9" pin="NC" pad="AB1"/>
<connect gate="NC90" pin="NC" pad="N1"/>
<connect gate="NC91" pin="NC" pad="N2"/>
<connect gate="NC92" pin="NC" pad="N21"/>
<connect gate="NC93" pin="NC" pad="N22"/>
<connect gate="NC94" pin="NC" pad="P2"/>
<connect gate="NC95" pin="NC" pad="P3"/>
<connect gate="NC96" pin="NC" pad="P20"/>
<connect gate="NC97" pin="NC" pad="P21"/>
<connect gate="NC98" pin="NC" pad="P22"/>
<connect gate="NC99" pin="NC" pad="R2"/>
<connect gate="V1" pin="VCC" pad="AA12"/>
<connect gate="V10" pin="VCC" pad="L10"/>
<connect gate="V11" pin="VCC" pad="L13"/>
<connect gate="V12" pin="VCC" pad="M10"/>
<connect gate="V13" pin="VCC" pad="M13"/>
<connect gate="V14" pin="VCC" pad="M14"/>
<connect gate="V15" pin="VCC" pad="N12"/>
<connect gate="V16" pin="VCC" pad="P8"/>
<connect gate="V17" pin="VCC" pad="P10"/>
<connect gate="V18" pin="VCC" pad="P12"/>
<connect gate="V19" pin="VCC" pad="P15"/>
<connect gate="V2" pin="VCC" pad="C11"/>
<connect gate="V20" pin="VCC" pad="R14"/>
<connect gate="V21" pin="VCC" pad="V5"/>
<connect gate="V22" pin="VCC" pad="W21"/>
<connect gate="V23" pin="VCC" pad="Y8"/>
<connect gate="V3" pin="VCC" pad="C15"/>
<connect gate="V4" pin="VCC" pad="H14"/>
<connect gate="V5" pin="VCC" pad="J8"/>
<connect gate="V6" pin="VCC" pad="J10"/>
<connect gate="V7" pin="VCC" pad="J12"/>
<connect gate="V8" pin="VCC" pad="J15"/>
<connect gate="V9" pin="VCC" pad="L9"/>
<connect gate="VO1" pin="VCCIO" pad="AB13"/>
<connect gate="VO10" pin="VCCIO" pad="J11"/>
<connect gate="VO11" pin="VCCIO" pad="J13"/>
<connect gate="VO12" pin="VCCIO" pad="K9"/>
<connect gate="VO13" pin="VCCIO" pad="K11"/>
<connect gate="VO14" pin="VCCIO" pad="K14"/>
<connect gate="VO15" pin="VCCIO" pad="K20"/>
<connect gate="VO16" pin="VCCIO" pad="L14"/>
<connect gate="VO17" pin="VCCIO" pad="M9"/>
<connect gate="VO18" pin="VCCIO" pad="N3"/>
<connect gate="VO19" pin="VCCIO" pad="N9"/>
<connect gate="VO2" pin="VCCIO" pad="A6"/>
<connect gate="VO20" pin="VCCIO" pad="N11"/>
<connect gate="VO21" pin="VCCIO" pad="N14"/>
<connect gate="VO22" pin="VCCIO" pad="N20"/>
<connect gate="VO23" pin="VCCIO" pad="P13"/>
<connect gate="VO24" pin="VCCIO" pad="R1"/>
<connect gate="VO25" pin="VCCIO" pad="R9"/>
<connect gate="VO26" pin="VCCIO" pad="T3"/>
<connect gate="VO27" pin="VCCIO" pad="T15"/>
<connect gate="VO28" pin="VCCIO" pad="T22"/>
<connect gate="VO29" pin="VCCIO" pad="V22"/>
<connect gate="VO3" pin="VCCIO" pad="A13"/>
<connect gate="VO4" pin="VCCIO" pad="B5"/>
<connect gate="VO5" pin="VCCIO" pad="E1"/>
<connect gate="VO6" pin="VCCIO" pad="G1"/>
<connect gate="VO7" pin="VCCIO" pad="G15"/>
<connect gate="VO8" pin="VCCIO" pad="H9"/>
<connect gate="VO9" pin="VCCIO" pad="H20"/>
<connect gate="_" pin="/CE" pad="E4"/>
<connect gate="_" pin="/CEO" pad="E19"/>
<connect gate="_" pin="/CONFIG" pad="T7"/>
<connect gate="_" pin="/STATUS" pad="W19"/>
<connect gate="_" pin="CONF_DONE" pad="F18"/>
<connect gate="_" pin="DATA0" pad="D4"/>
<connect gate="_" pin="DCLK" pad="E5"/>
<connect gate="_" pin="GCLK0" pad="P11"/>
<connect gate="_" pin="GCLK1" pad="D12"/>
<connect gate="_" pin="IN0" pad="R12"/>
<connect gate="_" pin="IN1" pad="V11"/>
<connect gate="_" pin="IN2" pad="H11"/>
<connect gate="_" pin="IN3" pad="E12"/>
<connect gate="_" pin="MSEL0" pad="U4"/>
<connect gate="_" pin="MSEL1" pad="V4"/>
<connect gate="_" pin="TCK" pad="E18"/>
<connect gate="_" pin="TDI" pad="F5"/>
<connect gate="_" pin="TDO" pad="F19"/>
<connect gate="_" pin="TMS" pad="U18"/>
<connect gate="_" pin="TRST" pad="V19"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30AFC484-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8942"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30-FBGA256" prefix="IC">
<description>&lt;b&gt;EPF10K30&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A16-30B"/>
<gate name="-B" symbol="B16-30B"/>
<gate name="-C" symbol="C16-30B"/>
<gate name="-D" symbol="D16-30B"/>
<gate name="-E" symbol="E16-30B"/>
<gate name="-F" symbol="F14-30B"/>
<gate name="-1" symbol="71-30B"/>
<gate name="-2" symbol="124-30B"/>
<gate name="-3" symbol="181-30B"/>
<gate name="-4" symbol="231-30B"/>
<gate name="-5" symbol="284-30B"/>
<gate name="-6" symbol="351-30B"/>
<gate name="-7" symbol="363-30B"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="FBGA256">
<connects>
<connect gate="-1" pin="IO11" pad="T1"/>
<connect gate="-1" pin="IO12" pad="B3"/>
<connect gate="-1" pin="IO21" pad="T3"/>
<connect gate="-1" pin="IO22" pad="T2"/>
<connect gate="-1" pin="IO23" pad="A2"/>
<connect gate="-1" pin="IO31" pad="P3"/>
<connect gate="-1" pin="IO32" pad="C3"/>
<connect gate="-1" pin="IO41" pad="R3"/>
<connect gate="-1" pin="IO42" pad="A3"/>
<connect gate="-1" pin="IO43" pad="B4"/>
<connect gate="-1" pin="IO52" pad="P4"/>
<connect gate="-1" pin="IO53" pad="A4"/>
<connect gate="-1" pin="IO61" pad="T4"/>
<connect gate="-1" pin="IO62" pad="C4"/>
<connect gate="-1" pin="IO63" pad="D4"/>
<connect gate="-1" pin="IO71" pad="N5"/>
<connect gate="-2" pin="IO101" pad="N6"/>
<connect gate="-2" pin="IO102" pad="D5"/>
<connect gate="-2" pin="IO104" pad="R5"/>
<connect gate="-2" pin="IO111" pad="P6"/>
<connect gate="-2" pin="IO112" pad="E4"/>
<connect gate="-2" pin="IO113" pad="B6"/>
<connect gate="-2" pin="IO121" pad="R6"/>
<connect gate="-2" pin="IO122" pad="T6"/>
<connect gate="-2" pin="IO123" pad="C6"/>
<connect gate="-2" pin="IO124" pad="A6"/>
<connect gate="-2" pin="IO72" pad="R4"/>
<connect gate="-2" pin="IO73" pad="B5"/>
<connect gate="-2" pin="IO81" pad="P5"/>
<connect gate="-2" pin="IO83" pad="A5"/>
<connect gate="-2" pin="IO91" pad="T5"/>
<connect gate="-2" pin="IO93" pad="C5"/>
<connect gate="-3" pin="IO131" pad="N7"/>
<connect gate="-3" pin="IO132" pad="M7"/>
<connect gate="-3" pin="IO133" pad="D6"/>
<connect gate="-3" pin="IO141" pad="T7"/>
<connect gate="-3" pin="IO142" pad="A7"/>
<connect gate="-3" pin="IO143" pad="B7"/>
<connect gate="-3" pin="IO144" pad="P7"/>
<connect gate="-3" pin="IO151" pad="R7"/>
<connect gate="-3" pin="IO152" pad="C7"/>
<connect gate="-3" pin="IO153" pad="D7"/>
<connect gate="-3" pin="IO161" pad="M8"/>
<connect gate="-3" pin="IO162" pad="E7"/>
<connect gate="-3" pin="IO171" pad="N8"/>
<connect gate="-3" pin="IO172" pad="A8"/>
<connect gate="-3" pin="IO173" pad="B8"/>
<connect gate="-3" pin="IO181" pad="P8"/>
<connect gate="-4" pin="IO182" pad="C8"/>
<connect gate="-4" pin="IO183" pad="D8"/>
<connect gate="-4" pin="IO191" pad="T9"/>
<connect gate="-4" pin="IO192" pad="R9"/>
<connect gate="-4" pin="IO193" pad="C9"/>
<connect gate="-4" pin="IO201" pad="N9"/>
<connect gate="-4" pin="IO202" pad="D9"/>
<connect gate="-4" pin="IO203" pad="E9"/>
<connect gate="-4" pin="IO204" pad="P9"/>
<connect gate="-4" pin="IO211" pad="R10"/>
<connect gate="-4" pin="IO212" pad="P10"/>
<connect gate="-4" pin="IO213" pad="A10"/>
<connect gate="-4" pin="IO221" pad="T10"/>
<connect gate="-4" pin="IO222" pad="B10"/>
<connect gate="-4" pin="IO223" pad="C10"/>
<connect gate="-4" pin="IO231" pad="N10"/>
<connect gate="-5" pin="IO232" pad="D10"/>
<connect gate="-5" pin="IO233" pad="E10"/>
<connect gate="-5" pin="IO241" pad="M10"/>
<connect gate="-5" pin="IO242" pad="A11"/>
<connect gate="-5" pin="IO251" pad="T11"/>
<connect gate="-5" pin="IO252" pad="R11"/>
<connect gate="-5" pin="IO253" pad="B11"/>
<connect gate="-5" pin="IO261" pad="N11"/>
<connect gate="-5" pin="IO262" pad="P11"/>
<connect gate="-5" pin="IO263" pad="D11"/>
<connect gate="-5" pin="IO264" pad="C11"/>
<connect gate="-5" pin="IO271" pad="R12"/>
<connect gate="-5" pin="IO272" pad="A12"/>
<connect gate="-5" pin="IO281" pad="P12"/>
<connect gate="-5" pin="IO282" pad="C12"/>
<connect gate="-5" pin="IO284" pad="B12"/>
<connect gate="-6" pin="IO291" pad="P14"/>
<connect gate="-6" pin="IO292" pad="T12"/>
<connect gate="-6" pin="IO293" pad="C13"/>
<connect gate="-6" pin="IO301" pad="P13"/>
<connect gate="-6" pin="IO303" pad="A13"/>
<connect gate="-6" pin="IO311" pad="T13"/>
<connect gate="-6" pin="IO313" pad="B13"/>
<connect gate="-6" pin="IO321" pad="R13"/>
<connect gate="-6" pin="IO322" pad="D13"/>
<connect gate="-6" pin="IO323" pad="D14"/>
<connect gate="-6" pin="IO331" pad="R14"/>
<connect gate="-6" pin="IO332" pad="C14"/>
<connect gate="-6" pin="IO341" pad="T14"/>
<connect gate="-6" pin="IO342" pad="A14"/>
<connect gate="-6" pin="IO343" pad="B14"/>
<connect gate="-6" pin="IO351" pad="T15"/>
<connect gate="-7" pin="IO352" pad="A15"/>
<connect gate="-7" pin="IO361" pad="R15"/>
<connect gate="-7" pin="IO362" pad="P16"/>
<connect gate="-7" pin="IO363" pad="A16"/>
<connect gate="-A" pin="IOA1" pad="E13"/>
<connect gate="-A" pin="IOA10" pad="E3"/>
<connect gate="-A" pin="IOA11" pad="D3"/>
<connect gate="-A" pin="IOA12" pad="D2"/>
<connect gate="-A" pin="IOA13" pad="C1"/>
<connect gate="-A" pin="IOA15" pad="D1"/>
<connect gate="-A" pin="IOA16" pad="F3"/>
<connect gate="-A" pin="IOA3" pad="E14"/>
<connect gate="-A" pin="IOA4" pad="D15"/>
<connect gate="-A" pin="IOA5" pad="D16"/>
<connect gate="-A" pin="IOA6" pad="F13"/>
<connect gate="-A" pin="IOA7" pad="E15"/>
<connect gate="-A" pin="IOA8" pad="E1"/>
<connect gate="-A" pin="IOA9" pad="F4"/>
<connect gate="-B" pin="IOB1" pad="E16"/>
<connect gate="-B" pin="IOB10" pad="F2"/>
<connect gate="-B" pin="IOB11" pad="F1"/>
<connect gate="-B" pin="IOB12" pad="G5"/>
<connect gate="-B" pin="IOB14" pad="E2"/>
<connect gate="-B" pin="IOB16" pad="G3"/>
<connect gate="-B" pin="IOB2" pad="F14"/>
<connect gate="-B" pin="IOB3" pad="G12"/>
<connect gate="-B" pin="IOB5" pad="G13"/>
<connect gate="-B" pin="IOB6" pad="F16"/>
<connect gate="-B" pin="IOB7" pad="F15"/>
<connect gate="-B" pin="IOB8" pad="H5"/>
<connect gate="-B" pin="IOB9" pad="G4"/>
<connect gate="-C" pin="IOC1" pad="G14"/>
<connect gate="-C" pin="IOC10" pad="H3"/>
<connect gate="-C" pin="IOC11" pad="H4"/>
<connect gate="-C" pin="IOC12" pad="G2"/>
<connect gate="-C" pin="IOC14" pad="G1"/>
<connect gate="-C" pin="IOC15" pad="H1"/>
<connect gate="-C" pin="IOC16" pad="H16"/>
<connect gate="-C" pin="IOC2" pad="H12"/>
<connect gate="-C" pin="IOC3" pad="G15"/>
<connect gate="-C" pin="IOC4" pad="G16"/>
<connect gate="-C" pin="IOC6" pad="H13"/>
<connect gate="-C" pin="IOC7" pad="H14"/>
<connect gate="-C" pin="IOC8" pad="J5"/>
<connect gate="-C" pin="IOC9" pad="H2"/>
<connect gate="-D" pin="IOD1" pad="H15"/>
<connect gate="-D" pin="IOD10" pad="J2"/>
<connect gate="-D" pin="IOD11" pad="J1"/>
<connect gate="-D" pin="IOD12" pad="J3"/>
<connect gate="-D" pin="IOD14" pad="J4"/>
<connect gate="-D" pin="IOD15" pad="K3"/>
<connect gate="-D" pin="IOD16" pad="K16"/>
<connect gate="-D" pin="IOD2" pad="J12"/>
<connect gate="-D" pin="IOD3" pad="J13"/>
<connect gate="-D" pin="IOD4" pad="J14"/>
<connect gate="-D" pin="IOD5" pad="J16"/>
<connect gate="-D" pin="IOD6" pad="J15"/>
<connect gate="-D" pin="IOD7" pad="K12"/>
<connect gate="-D" pin="IOD8" pad="K1"/>
<connect gate="-D" pin="IOD9" pad="K4"/>
<connect gate="-E" pin="IOE1" pad="K15"/>
<connect gate="-E" pin="IOE10" pad="L1"/>
<connect gate="-E" pin="IOE11" pad="L3"/>
<connect gate="-E" pin="IOE12" pad="K5"/>
<connect gate="-E" pin="IOE14" pad="K2"/>
<connect gate="-E" pin="IOE15" pad="L4"/>
<connect gate="-E" pin="IOE16" pad="M14"/>
<connect gate="-E" pin="IOE2" pad="K14"/>
<connect gate="-E" pin="IOE3" pad="K13"/>
<connect gate="-E" pin="IOE4" pad="L14"/>
<connect gate="-E" pin="IOE5" pad="L15"/>
<connect gate="-E" pin="IOE6" pad="L16"/>
<connect gate="-E" pin="IOE7" pad="L13"/>
<connect gate="-E" pin="IOE8" pad="M2"/>
<connect gate="-E" pin="IOE9" pad="L2"/>
<connect gate="-F" pin="IOF1" pad="M15"/>
<connect gate="-F" pin="IOF10" pad="N3"/>
<connect gate="-F" pin="IOF11" pad="N2"/>
<connect gate="-F" pin="IOF12" pad="M4"/>
<connect gate="-F" pin="IOF13" pad="M3"/>
<connect gate="-F" pin="IOF14" pad="M1"/>
<connect gate="-F" pin="IOF2" pad="M16"/>
<connect gate="-F" pin="IOF3" pad="M13"/>
<connect gate="-F" pin="IOF4" pad="N13"/>
<connect gate="-F" pin="IOF5" pad="N14"/>
<connect gate="-F" pin="IOF6" pad="N15"/>
<connect gate="-F" pin="IOF7" pad="N16"/>
<connect gate="-F" pin="IOF8" pad="P2"/>
<connect gate="-F" pin="IOF9" pad="N1"/>
<connect gate="G1" pin="GND" pad="E5"/>
<connect gate="G10" pin="GND" pad="J8"/>
<connect gate="G11" pin="GND" pad="J9"/>
<connect gate="G12" pin="GND" pad="K7"/>
<connect gate="G13" pin="GND" pad="K10"/>
<connect gate="G14" pin="GND" pad="L6"/>
<connect gate="G15" pin="GND" pad="L11"/>
<connect gate="G16" pin="GND" pad="M5"/>
<connect gate="G17" pin="GND" pad="M12"/>
<connect gate="G18" pin="GND" pad="T8"/>
<connect gate="G2" pin="GND" pad="E12"/>
<connect gate="G3" pin="GND" pad="F6"/>
<connect gate="G4" pin="GND" pad="F11"/>
<connect gate="G5" pin="GND" pad="G7"/>
<connect gate="G6" pin="GND" pad="G9"/>
<connect gate="G7" pin="GND" pad="G10"/>
<connect gate="G8" pin="GND" pad="H8"/>
<connect gate="G9" pin="GND" pad="H9"/>
<connect gate="V1" pin="VCC" pad="E11"/>
<connect gate="V10" pin="VCC" pad="J10"/>
<connect gate="V11" pin="VCC" pad="J11"/>
<connect gate="V12" pin="VCC" pad="K9"/>
<connect gate="V13" pin="VCC" pad="L5"/>
<connect gate="V14" pin="VCC" pad="L7"/>
<connect gate="V15" pin="VCC" pad="L9"/>
<connect gate="V16" pin="VCC" pad="L12"/>
<connect gate="V17" pin="VCC" pad="M11"/>
<connect gate="V18" pin="VCC" pad="R2"/>
<connect gate="V2" pin="VCC" pad="F5"/>
<connect gate="V3" pin="VCC" pad="F7"/>
<connect gate="V4" pin="VCC" pad="F9"/>
<connect gate="V5" pin="VCC" pad="F12"/>
<connect gate="V6" pin="VCC" pad="H6"/>
<connect gate="V7" pin="VCC" pad="H7"/>
<connect gate="V8" pin="VCC" pad="H10"/>
<connect gate="V9" pin="VCC" pad="J7"/>
<connect gate="VO1" pin="VCCIO" pad="D12"/>
<connect gate="VO10" pin="VCCIO" pad="K6"/>
<connect gate="VO11" pin="VCCIO" pad="K8"/>
<connect gate="VO12" pin="VCCIO" pad="K11"/>
<connect gate="VO13" pin="VCCIO" pad="L10"/>
<connect gate="VO14" pin="VCCIO" pad="M6"/>
<connect gate="VO15" pin="VCCIO" pad="N12"/>
<connect gate="VO2" pin="VCCIO" pad="E6"/>
<connect gate="VO3" pin="VCCIO" pad="F8"/>
<connect gate="VO4" pin="VCCIO" pad="F10"/>
<connect gate="VO5" pin="VCCIO" pad="G6"/>
<connect gate="VO6" pin="VCCIO" pad="G8"/>
<connect gate="VO7" pin="VCCIO" pad="G11"/>
<connect gate="VO8" pin="VCCIO" pad="H11"/>
<connect gate="VO9" pin="VCCIO" pad="J6"/>
<connect gate="_" pin="/CE" pad="B1"/>
<connect gate="_" pin="/CEO" pad="B16"/>
<connect gate="_" pin="/CONFIG" pad="N4"/>
<connect gate="_" pin="/STATUS" pad="T16"/>
<connect gate="_" pin="CONF_DONE" pad="C15"/>
<connect gate="_" pin="DATA0" pad="A1"/>
<connect gate="_" pin="DCLK" pad="B2"/>
<connect gate="_" pin="GCLK0" pad="L8"/>
<connect gate="_" pin="GCLK1" pad="A9"/>
<connect gate="_" pin="IN0" pad="M9"/>
<connect gate="_" pin="IN1" pad="R8"/>
<connect gate="_" pin="IN2" pad="E8"/>
<connect gate="_" pin="IN3" pad="B9"/>
<connect gate="_" pin="MSEL0" pad="P1"/>
<connect gate="_" pin="MSEL1" pad="R1"/>
<connect gate="_" pin="TCK" pad="B15"/>
<connect gate="_" pin="TDI" pad="C2"/>
<connect gate="_" pin="TDO" pad="C16"/>
<connect gate="_" pin="TMS" pad="P15"/>
<connect gate="_" pin="TRST" pad="R16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30EFC256-3N"/>
<attribute name="OC_FARNELL" value="1549394"/>
<attribute name="OC_NEWARK" value="51R8977"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30*-FBGA256" prefix="IC">
<description>&lt;b&gt;EPF10K30&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A12"/>
<gate name="-B" symbol="B11"/>
<gate name="-C" symbol="C12"/>
<gate name="-D" symbol="D12"/>
<gate name="-E" symbol="E11"/>
<gate name="-F" symbol="F12"/>
<gate name="-1" symbol="71-K30EF"/>
<gate name="-2" symbol="124-K30E"/>
<gate name="-3" symbol="181-K30E"/>
<gate name="-4" symbol="231-K30E"/>
<gate name="-5" symbol="281-K30E"/>
<gate name="-6" symbol="351-K30E"/>
<gate name="-7" symbol="363-K30E"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="G15" symbol="GND"/>
<gate name="G16" symbol="GND"/>
<gate name="G17" symbol="GND"/>
<gate name="G18" symbol="GND"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="V17" symbol="VCCINT"/>
<gate name="V18" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="FBGA256">
<connects>
<connect gate="-1" pin="IO11" pad="T1"/>
<connect gate="-1" pin="IO12" pad="B3"/>
<connect gate="-1" pin="IO21" pad="T3"/>
<connect gate="-1" pin="IO22" pad="A2"/>
<connect gate="-1" pin="IO23" pad="T2"/>
<connect gate="-1" pin="IO31" pad="P3"/>
<connect gate="-1" pin="IO32" pad="C3"/>
<connect gate="-1" pin="IO41" pad="R3"/>
<connect gate="-1" pin="IO42" pad="A3"/>
<connect gate="-1" pin="IO43" pad="B4"/>
<connect gate="-1" pin="IO51" pad="P4"/>
<connect gate="-1" pin="IO52" pad="A4"/>
<connect gate="-1" pin="IO61" pad="T4"/>
<connect gate="-1" pin="IO62" pad="C4"/>
<connect gate="-1" pin="IO63" pad="D4"/>
<connect gate="-1" pin="IO71" pad="N5"/>
<connect gate="-2" pin="IO101" pad="N6"/>
<connect gate="-2" pin="IO102" pad="D5"/>
<connect gate="-2" pin="IO103" pad="R5"/>
<connect gate="-2" pin="IO111" pad="P6"/>
<connect gate="-2" pin="IO112" pad="B6"/>
<connect gate="-2" pin="IO113" pad="E4"/>
<connect gate="-2" pin="IO121" pad="R6"/>
<connect gate="-2" pin="IO122" pad="C6"/>
<connect gate="-2" pin="IO123" pad="A6"/>
<connect gate="-2" pin="IO124" pad="T6"/>
<connect gate="-2" pin="IO72" pad="B5"/>
<connect gate="-2" pin="IO73" pad="R4"/>
<connect gate="-2" pin="IO81" pad="P5"/>
<connect gate="-2" pin="IO82" pad="A5"/>
<connect gate="-2" pin="IO91" pad="T5"/>
<connect gate="-2" pin="IO93" pad="C5"/>
<connect gate="-3" pin="IO131" pad="N7"/>
<connect gate="-3" pin="IO132" pad="D6"/>
<connect gate="-3" pin="IO133" pad="M7"/>
<connect gate="-3" pin="IO141" pad="T7"/>
<connect gate="-3" pin="IO142" pad="P7"/>
<connect gate="-3" pin="IO143" pad="A7"/>
<connect gate="-3" pin="IO144" pad="B7"/>
<connect gate="-3" pin="IO151" pad="R7"/>
<connect gate="-3" pin="IO152" pad="D7"/>
<connect gate="-3" pin="IO153" pad="C7"/>
<connect gate="-3" pin="IO161" pad="M8"/>
<connect gate="-3" pin="IO162" pad="E7"/>
<connect gate="-3" pin="IO171" pad="N8"/>
<connect gate="-3" pin="IO172" pad="B8"/>
<connect gate="-3" pin="IO173" pad="A8"/>
<connect gate="-3" pin="IO181" pad="D8"/>
<connect gate="-4" pin="IO182" pad="C8"/>
<connect gate="-4" pin="IO183" pad="P8"/>
<connect gate="-4" pin="IO191" pad="T9"/>
<connect gate="-4" pin="IO192" pad="C9"/>
<connect gate="-4" pin="IO193" pad="R9"/>
<connect gate="-4" pin="IO201" pad="N9"/>
<connect gate="-4" pin="IO202" pad="P9"/>
<connect gate="-4" pin="IO203" pad="E9"/>
<connect gate="-4" pin="IO204" pad="D9"/>
<connect gate="-4" pin="IO211" pad="R10"/>
<connect gate="-4" pin="IO212" pad="A10"/>
<connect gate="-4" pin="IO213" pad="P10"/>
<connect gate="-4" pin="IO221" pad="T10"/>
<connect gate="-4" pin="IO222" pad="C10"/>
<connect gate="-4" pin="IO223" pad="B10"/>
<connect gate="-4" pin="IO231" pad="N10"/>
<connect gate="-5" pin="IO232" pad="E10"/>
<connect gate="-5" pin="IO233" pad="D10"/>
<connect gate="-5" pin="IO241" pad="M10"/>
<connect gate="-5" pin="IO242" pad="A11"/>
<connect gate="-5" pin="IO251" pad="T11"/>
<connect gate="-5" pin="IO252" pad="B11"/>
<connect gate="-5" pin="IO253" pad="R11"/>
<connect gate="-5" pin="IO261" pad="N11"/>
<connect gate="-5" pin="IO262" pad="P11"/>
<connect gate="-5" pin="IO263" pad="D11"/>
<connect gate="-5" pin="IO264" pad="C11"/>
<connect gate="-5" pin="IO271" pad="R12"/>
<connect gate="-5" pin="IO273" pad="A12"/>
<connect gate="-5" pin="IO281" pad="P12"/>
<connect gate="-5" pin="IO282" pad="B12"/>
<connect gate="-5" pin="IO283" pad="C12"/>
<connect gate="-6" pin="IO291" pad="T12"/>
<connect gate="-6" pin="IO292" pad="C13"/>
<connect gate="-6" pin="IO293" pad="P14"/>
<connect gate="-6" pin="IO301" pad="P13"/>
<connect gate="-6" pin="IO302" pad="A13"/>
<connect gate="-6" pin="IO311" pad="T13"/>
<connect gate="-6" pin="IO312" pad="B13"/>
<connect gate="-6" pin="IO321" pad="R13"/>
<connect gate="-6" pin="IO322" pad="D14"/>
<connect gate="-6" pin="IO323" pad="D13"/>
<connect gate="-6" pin="IO331" pad="R14"/>
<connect gate="-6" pin="IO332" pad="C14"/>
<connect gate="-6" pin="IO341" pad="T14"/>
<connect gate="-6" pin="IO342" pad="A14"/>
<connect gate="-6" pin="IO343" pad="B14"/>
<connect gate="-6" pin="IO351" pad="T15"/>
<connect gate="-7" pin="IO352" pad="A15"/>
<connect gate="-7" pin="IO361" pad="R15"/>
<connect gate="-7" pin="IO362" pad="A16"/>
<connect gate="-7" pin="IO363" pad="P16"/>
<connect gate="-A" pin="IOA1" pad="E13"/>
<connect gate="-A" pin="IOA10" pad="D3"/>
<connect gate="-A" pin="IOA11" pad="F3"/>
<connect gate="-A" pin="IOA12" pad="F13"/>
<connect gate="-A" pin="IOA2" pad="E14"/>
<connect gate="-A" pin="IOA3" pad="D16"/>
<connect gate="-A" pin="IOA4" pad="D15"/>
<connect gate="-A" pin="IOA5" pad="E15"/>
<connect gate="-A" pin="IOA6" pad="E1"/>
<connect gate="-A" pin="IOA7" pad="F4"/>
<connect gate="-A" pin="IOA8" pad="D2"/>
<connect gate="-A" pin="IOA9" pad="C1"/>
<connect gate="-B" pin="IOB1" pad="F14"/>
<connect gate="-B" pin="IOB10" pad="E2"/>
<connect gate="-B" pin="IOB11" pad="F16"/>
<connect gate="-B" pin="IOB2" pad="G12"/>
<connect gate="-B" pin="IOB3" pad="G13"/>
<connect gate="-B" pin="IOB4" pad="F15"/>
<connect gate="-B" pin="IOB5" pad="H5"/>
<connect gate="-B" pin="IOB6" pad="G4"/>
<connect gate="-B" pin="IOB7" pad="F2"/>
<connect gate="-B" pin="IOB8" pad="F1"/>
<connect gate="-B" pin="IOB9" pad="G5"/>
<connect gate="-C" pin="IOC1" pad="G14"/>
<connect gate="-C" pin="IOC10" pad="G2"/>
<connect gate="-C" pin="IOC11" pad="G1"/>
<connect gate="-C" pin="IOC12" pad="H13"/>
<connect gate="-C" pin="IOC2" pad="H12"/>
<connect gate="-C" pin="IOC3" pad="G15"/>
<connect gate="-C" pin="IOC4" pad="G16"/>
<connect gate="-C" pin="IOC5" pad="H14"/>
<connect gate="-C" pin="IOC6" pad="J5"/>
<connect gate="-C" pin="IOC7" pad="H2"/>
<connect gate="-C" pin="IOC8" pad="H3"/>
<connect gate="-C" pin="IOC9" pad="H4"/>
<connect gate="-D" pin="IOD1" pad="H15"/>
<connect gate="-D" pin="IOD10" pad="J3"/>
<connect gate="-D" pin="IOD11" pad="J4"/>
<connect gate="-D" pin="IOD12" pad="K4"/>
<connect gate="-D" pin="IOD2" pad="J12"/>
<connect gate="-D" pin="IOD3" pad="J13"/>
<connect gate="-D" pin="IOD4" pad="J14"/>
<connect gate="-D" pin="IOD5" pad="J16"/>
<connect gate="-D" pin="IOD6" pad="J15"/>
<connect gate="-D" pin="IOD7" pad="K12"/>
<connect gate="-D" pin="IOD8" pad="K1"/>
<connect gate="-D" pin="IOD9" pad="J2"/>
<connect gate="-E" pin="IOE1" pad="K15"/>
<connect gate="-E" pin="IOE10" pad="K2"/>
<connect gate="-E" pin="IOE11" pad="L3"/>
<connect gate="-E" pin="IOE2" pad="K13"/>
<connect gate="-E" pin="IOE3" pad="L14"/>
<connect gate="-E" pin="IOE4" pad="L15"/>
<connect gate="-E" pin="IOE5" pad="L16"/>
<connect gate="-E" pin="IOE6" pad="L13"/>
<connect gate="-E" pin="IOE7" pad="M2"/>
<connect gate="-E" pin="IOE8" pad="L1"/>
<connect gate="-E" pin="IOE9" pad="K5"/>
<connect gate="-F" pin="IOF1" pad="M15"/>
<connect gate="-F" pin="IOF10" pad="M1"/>
<connect gate="-F" pin="IOF11" pad="M3"/>
<connect gate="-F" pin="IOF12" pad="N13"/>
<connect gate="-F" pin="IOF2" pad="M13"/>
<connect gate="-F" pin="IOF3" pad="N14"/>
<connect gate="-F" pin="IOF4" pad="N16"/>
<connect gate="-F" pin="IOF5" pad="P2"/>
<connect gate="-F" pin="IOF6" pad="N1"/>
<connect gate="-F" pin="IOF7" pad="N3"/>
<connect gate="-F" pin="IOF8" pad="N2"/>
<connect gate="-F" pin="IOF9" pad="M4"/>
<connect gate="G1" pin="GND" pad="E5"/>
<connect gate="G10" pin="GND" pad="J8"/>
<connect gate="G11" pin="GND" pad="J9"/>
<connect gate="G12" pin="GND" pad="K7"/>
<connect gate="G13" pin="GND" pad="K10"/>
<connect gate="G14" pin="GND" pad="L6"/>
<connect gate="G15" pin="GND" pad="L11"/>
<connect gate="G16" pin="GND" pad="M5"/>
<connect gate="G17" pin="GND" pad="M12"/>
<connect gate="G18" pin="GND" pad="T8"/>
<connect gate="G2" pin="GND" pad="E12"/>
<connect gate="G3" pin="GND" pad="F6"/>
<connect gate="G4" pin="GND" pad="F11"/>
<connect gate="G5" pin="GND" pad="G7"/>
<connect gate="G6" pin="GND" pad="G9"/>
<connect gate="G7" pin="GND" pad="G10"/>
<connect gate="G8" pin="GND" pad="H8"/>
<connect gate="G9" pin="GND" pad="H9"/>
<connect gate="NC1" pin="NC" pad="D1"/>
<connect gate="NC10" pin="NC" pad="K16"/>
<connect gate="NC11" pin="NC" pad="L2"/>
<connect gate="NC12" pin="NC" pad="L4"/>
<connect gate="NC13" pin="NC" pad="M14"/>
<connect gate="NC14" pin="NC" pad="M16"/>
<connect gate="NC15" pin="NC" pad="N15"/>
<connect gate="NC2" pin="NC" pad="E3"/>
<connect gate="NC3" pin="NC" pad="E16"/>
<connect gate="NC4" pin="NC" pad="G3"/>
<connect gate="NC5" pin="NC" pad="H1"/>
<connect gate="NC6" pin="NC" pad="H16"/>
<connect gate="NC7" pin="NC" pad="J1"/>
<connect gate="NC8" pin="NC" pad="K3"/>
<connect gate="NC9" pin="NC" pad="K14"/>
<connect gate="V1" pin="VCC" pad="E11"/>
<connect gate="V10" pin="VCC" pad="J10"/>
<connect gate="V11" pin="VCC" pad="J11"/>
<connect gate="V12" pin="VCC" pad="K9"/>
<connect gate="V13" pin="VCC" pad="L5"/>
<connect gate="V14" pin="VCC" pad="L7"/>
<connect gate="V15" pin="VCC" pad="L9"/>
<connect gate="V16" pin="VCC" pad="L12"/>
<connect gate="V17" pin="VCC" pad="M11"/>
<connect gate="V18" pin="VCC" pad="R2"/>
<connect gate="V2" pin="VCC" pad="F5"/>
<connect gate="V3" pin="VCC" pad="F7"/>
<connect gate="V4" pin="VCC" pad="F9"/>
<connect gate="V5" pin="VCC" pad="F12"/>
<connect gate="V6" pin="VCC" pad="H6"/>
<connect gate="V7" pin="VCC" pad="H7"/>
<connect gate="V8" pin="VCC" pad="H10"/>
<connect gate="V9" pin="VCC" pad="J7"/>
<connect gate="VO1" pin="VCCIO" pad="D12"/>
<connect gate="VO10" pin="VCCIO" pad="K6"/>
<connect gate="VO11" pin="VCCIO" pad="K8"/>
<connect gate="VO12" pin="VCCIO" pad="K11"/>
<connect gate="VO13" pin="VCCIO" pad="L10"/>
<connect gate="VO14" pin="VCCIO" pad="M6"/>
<connect gate="VO15" pin="VCCIO" pad="N12"/>
<connect gate="VO2" pin="VCCIO" pad="E6"/>
<connect gate="VO3" pin="VCCIO" pad="F8"/>
<connect gate="VO4" pin="VCCIO" pad="F10"/>
<connect gate="VO5" pin="VCCIO" pad="G6"/>
<connect gate="VO6" pin="VCCIO" pad="G8"/>
<connect gate="VO7" pin="VCCIO" pad="G11"/>
<connect gate="VO8" pin="VCCIO" pad="H11"/>
<connect gate="VO9" pin="VCCIO" pad="J6"/>
<connect gate="_" pin="/CE" pad="B1"/>
<connect gate="_" pin="/CEO" pad="B16"/>
<connect gate="_" pin="/CONFIG" pad="N4"/>
<connect gate="_" pin="/STATUS" pad="T16"/>
<connect gate="_" pin="CONF_DONE" pad="C15"/>
<connect gate="_" pin="DATA0" pad="A1"/>
<connect gate="_" pin="DCLK" pad="B2"/>
<connect gate="_" pin="GCLK0" pad="L8"/>
<connect gate="_" pin="GCLK1" pad="A9"/>
<connect gate="_" pin="IN0" pad="M9"/>
<connect gate="_" pin="IN1" pad="R8"/>
<connect gate="_" pin="IN2" pad="E8"/>
<connect gate="_" pin="IN3" pad="B9"/>
<connect gate="_" pin="MSEL0" pad="P1"/>
<connect gate="_" pin="MSEL1" pad="R1"/>
<connect gate="_" pin="TCK" pad="B15"/>
<connect gate="_" pin="TDI" pad="C2"/>
<connect gate="_" pin="TDO" pad="C16"/>
<connect gate="_" pin="TMS" pad="P15"/>
<connect gate="_" pin="TRST" pad="R16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30EFC256-3N"/>
<attribute name="OC_FARNELL" value="1549394"/>
<attribute name="OC_NEWARK" value="51R8977"/>
</technology>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30AQC240-3N"/>
<attribute name="OC_FARNELL" value="1549384"/>
<attribute name="OC_NEWARK" value="51R8956"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30-Q240" prefix="IC">
<description>&lt;b&gt;EPF10K30&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A13"/>
<gate name="-B" symbol="B14"/>
<gate name="-C" symbol="C14"/>
<gate name="-D" symbol="D14"/>
<gate name="-E" symbol="E14"/>
<gate name="-F" symbol="F14"/>
<gate name="-1" symbol="63-K30Q"/>
<gate name="-2" symbol="122-K30Q"/>
<gate name="-3" symbol="181-K30Q"/>
<gate name="-4" symbol="232-K30Q"/>
<gate name="-5" symbol="292-K30Q"/>
<gate name="-6" symbol="351-K30Q"/>
<gate name="-7" symbol="363-K30Q"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCINT"/>
<gate name="14" symbol="VCCINT"/>
<gate name="15" symbol="VCCINT"/>
<gate name="16" symbol="VCCINT"/>
<gate name="17" symbol="VCCINT"/>
<gate name="18" symbol="VCCINT"/>
<gate name="19" symbol="VCCINT"/>
<gate name="20" symbol="GNDINT"/>
<gate name="21" symbol="GNDINT"/>
<gate name="22" symbol="GNDINT"/>
<gate name="23" symbol="GNDINT"/>
<gate name="24" symbol="GNDINT"/>
<gate name="25" symbol="GNDINT"/>
<gate name="26" symbol="GNDINT"/>
<gate name="27" symbol="GNDINT"/>
<gate name="28" symbol="GNDINT"/>
<gate name="29" symbol="GNDINT"/>
<gate name="30" symbol="GNDINT"/>
<gate name="31" symbol="GNDINT"/>
<gate name="32" symbol="GNDINT"/>
<gate name="33" symbol="GNDINT"/>
<gate name="34" symbol="GNDINT"/>
<gate name="35" symbol="GNDINT"/>
<gate name="36" symbol="GNDINT"/>
<gate name="37" symbol="GNDINT"/>
</gates>
<devices>
<device name="" package="PQFP240">
<connects>
<connect gate="-1" pin="IO11" pad="120"/>
<connect gate="-1" pin="IO12" pad="181"/>
<connect gate="-1" pin="IO21" pad="118"/>
<connect gate="-1" pin="IO22" pad="119"/>
<connect gate="-1" pin="IO23" pad="182"/>
<connect gate="-1" pin="IO31" pad="117"/>
<connect gate="-1" pin="IO32" pad="183"/>
<connect gate="-1" pin="IO41" pad="116"/>
<connect gate="-1" pin="IO42" pad="184"/>
<connect gate="-1" pin="IO43" pad="185"/>
<connect gate="-1" pin="IO51" pad="114"/>
<connect gate="-1" pin="IO52" pad="115"/>
<connect gate="-1" pin="IO53" pad="186"/>
<connect gate="-1" pin="IO61" pad="113"/>
<connect gate="-1" pin="IO62" pad="187"/>
<connect gate="-1" pin="IO63" pad="188"/>
<connect gate="-2" pin="IO101" pad="106"/>
<connect gate="-2" pin="IO102" pad="194"/>
<connect gate="-2" pin="IO111" pad="105"/>
<connect gate="-2" pin="IO112" pad="195"/>
<connect gate="-2" pin="IO113" pad="196"/>
<connect gate="-2" pin="IO121" pad="102"/>
<connect gate="-2" pin="IO122" pad="103"/>
<connect gate="-2" pin="IO71" pad="110"/>
<connect gate="-2" pin="IO72" pad="111"/>
<connect gate="-2" pin="IO73" pad="190"/>
<connect gate="-2" pin="IO81" pad="109"/>
<connect gate="-2" pin="IO82" pad="191"/>
<connect gate="-2" pin="IO83" pad="192"/>
<connect gate="-2" pin="IO91" pad="107"/>
<connect gate="-2" pin="IO92" pad="108"/>
<connect gate="-2" pin="IO93" pad="193"/>
<connect gate="-3" pin="IO123" pad="198"/>
<connect gate="-3" pin="IO131" pad="100"/>
<connect gate="-3" pin="IO132" pad="101"/>
<connect gate="-3" pin="IO133" pad="199"/>
<connect gate="-3" pin="IO141" pad="99"/>
<connect gate="-3" pin="IO142" pad="200"/>
<connect gate="-3" pin="IO143" pad="201"/>
<connect gate="-3" pin="IO151" pad="98"/>
<connect gate="-3" pin="IO152" pad="202"/>
<connect gate="-3" pin="IO153" pad="203"/>
<connect gate="-3" pin="IO161" pad="97"/>
<connect gate="-3" pin="IO162" pad="204"/>
<connect gate="-3" pin="IO171" pad="95"/>
<connect gate="-3" pin="IO172" pad="206"/>
<connect gate="-3" pin="IO173" pad="207"/>
<connect gate="-3" pin="IO181" pad="94"/>
<connect gate="-4" pin="IO182" pad="208"/>
<connect gate="-4" pin="IO183" pad="209"/>
<connect gate="-4" pin="IO191" pad="87"/>
<connect gate="-4" pin="IO192" pad="88"/>
<connect gate="-4" pin="IO193" pad="213"/>
<connect gate="-4" pin="IO201" pad="86"/>
<connect gate="-4" pin="IO202" pad="214"/>
<connect gate="-4" pin="IO203" pad="215"/>
<connect gate="-4" pin="IO211" pad="83"/>
<connect gate="-4" pin="IO212" pad="84"/>
<connect gate="-4" pin="IO213" pad="217"/>
<connect gate="-4" pin="IO221" pad="82"/>
<connect gate="-4" pin="IO222" pad="218"/>
<connect gate="-4" pin="IO223" pad="219"/>
<connect gate="-4" pin="IO231" pad="81"/>
<connect gate="-4" pin="IO232" pad="220"/>
<connect gate="-5" pin="IO233" pad="221"/>
<connect gate="-5" pin="IO241" pad="80"/>
<connect gate="-5" pin="IO242" pad="222"/>
<connect gate="-5" pin="IO251" pad="78"/>
<connect gate="-5" pin="IO252" pad="79"/>
<connect gate="-5" pin="IO253" pad="223"/>
<connect gate="-5" pin="IO261" pad="75"/>
<connect gate="-5" pin="IO262" pad="76"/>
<connect gate="-5" pin="IO263" pad="225"/>
<connect gate="-5" pin="IO271" pad="74"/>
<connect gate="-5" pin="IO272" pad="226"/>
<connect gate="-5" pin="IO273" pad="227"/>
<connect gate="-5" pin="IO281" pad="73"/>
<connect gate="-5" pin="IO282" pad="228"/>
<connect gate="-5" pin="IO291" pad="71"/>
<connect gate="-5" pin="IO292" pad="72"/>
<connect gate="-6" pin="IO293" pad="229"/>
<connect gate="-6" pin="IO301" pad="70"/>
<connect gate="-6" pin="IO302" pad="230"/>
<connect gate="-6" pin="IO303" pad="231"/>
<connect gate="-6" pin="IO311" pad="67"/>
<connect gate="-6" pin="IO312" pad="68"/>
<connect gate="-6" pin="IO313" pad="233"/>
<connect gate="-6" pin="IO321" pad="66"/>
<connect gate="-6" pin="IO322" pad="234"/>
<connect gate="-6" pin="IO323" pad="235"/>
<connect gate="-6" pin="IO331" pad="65"/>
<connect gate="-6" pin="IO332" pad="236"/>
<connect gate="-6" pin="IO341" pad="64"/>
<connect gate="-6" pin="IO342" pad="237"/>
<connect gate="-6" pin="IO343" pad="238"/>
<connect gate="-6" pin="IO351" pad="63"/>
<connect gate="-7" pin="IO352" pad="239"/>
<connect gate="-7" pin="IO361" pad="61"/>
<connect gate="-7" pin="IO362" pad="62"/>
<connect gate="-7" pin="IO363" pad="240"/>
<connect gate="-A" pin="IOA1" pad="6"/>
<connect gate="-A" pin="IOA10" pad="172"/>
<connect gate="-A" pin="IOA11" pad="173"/>
<connect gate="-A" pin="IOA12" pad="174"/>
<connect gate="-A" pin="IOA13" pad="175"/>
<connect gate="-A" pin="IOA2" pad="7"/>
<connect gate="-A" pin="IOA3" pad="8"/>
<connect gate="-A" pin="IOA4" pad="9"/>
<connect gate="-A" pin="IOA5" pad="11"/>
<connect gate="-A" pin="IOA6" pad="12"/>
<connect gate="-A" pin="IOA7" pad="13"/>
<connect gate="-A" pin="IOA8" pad="169"/>
<connect gate="-A" pin="IOA9" pad="171"/>
<connect gate="-B" pin="IOB1" pad="14"/>
<connect gate="-B" pin="IOB10" pad="163"/>
<connect gate="-B" pin="IOB11" pad="164"/>
<connect gate="-B" pin="IOB12" pad="166"/>
<connect gate="-B" pin="IOB13" pad="167"/>
<connect gate="-B" pin="IOB14" pad="168"/>
<connect gate="-B" pin="IOB2" pad="15"/>
<connect gate="-B" pin="IOB3" pad="17"/>
<connect gate="-B" pin="IOB4" pad="18"/>
<connect gate="-B" pin="IOB5" pad="19"/>
<connect gate="-B" pin="IOB6" pad="20"/>
<connect gate="-B" pin="IOB7" pad="21"/>
<connect gate="-B" pin="IOB8" pad="161"/>
<connect gate="-B" pin="IOB9" pad="162"/>
<connect gate="-C" pin="IOC1" pad="23"/>
<connect gate="-C" pin="IOC10" pad="154"/>
<connect gate="-C" pin="IOC11" pad="156"/>
<connect gate="-C" pin="IOC12" pad="157"/>
<connect gate="-C" pin="IOC13" pad="158"/>
<connect gate="-C" pin="IOC14" pad="159"/>
<connect gate="-C" pin="IOC2" pad="24"/>
<connect gate="-C" pin="IOC3" pad="25"/>
<connect gate="-C" pin="IOC4" pad="26"/>
<connect gate="-C" pin="IOC5" pad="28"/>
<connect gate="-C" pin="IOC6" pad="29"/>
<connect gate="-C" pin="IOC7" pad="30"/>
<connect gate="-C" pin="IOC8" pad="152"/>
<connect gate="-C" pin="IOC9" pad="153"/>
<connect gate="-D" pin="IOD1" pad="31"/>
<connect gate="-D" pin="IOD10" pad="146"/>
<connect gate="-D" pin="IOD11" pad="147"/>
<connect gate="-D" pin="IOD12" pad="148"/>
<connect gate="-D" pin="IOD13" pad="149"/>
<connect gate="-D" pin="IOD14" pad="151"/>
<connect gate="-D" pin="IOD2" pad="33"/>
<connect gate="-D" pin="IOD3" pad="34"/>
<connect gate="-D" pin="IOD4" pad="35"/>
<connect gate="-D" pin="IOD5" pad="36"/>
<connect gate="-D" pin="IOD6" pad="38"/>
<connect gate="-D" pin="IOD7" pad="39"/>
<connect gate="-D" pin="IOD8" pad="143"/>
<connect gate="-D" pin="IOD9" pad="144"/>
<connect gate="-E" pin="IOE1" pad="40"/>
<connect gate="-E" pin="IOE10" pad="137"/>
<connect gate="-E" pin="IOE11" pad="138"/>
<connect gate="-E" pin="IOE12" pad="139"/>
<connect gate="-E" pin="IOE13" pad="141"/>
<connect gate="-E" pin="IOE14" pad="142"/>
<connect gate="-E" pin="IOE2" pad="41"/>
<connect gate="-E" pin="IOE3" pad="43"/>
<connect gate="-E" pin="IOE4" pad="44"/>
<connect gate="-E" pin="IOE5" pad="45"/>
<connect gate="-E" pin="IOE6" pad="46"/>
<connect gate="-E" pin="IOE7" pad="48"/>
<connect gate="-E" pin="IOE8" pad="134"/>
<connect gate="-E" pin="IOE9" pad="136"/>
<connect gate="-F" pin="IOF1" pad="49"/>
<connect gate="-F" pin="IOF10" pad="128"/>
<connect gate="-F" pin="IOF11" pad="129"/>
<connect gate="-F" pin="IOF12" pad="131"/>
<connect gate="-F" pin="IOF13" pad="132"/>
<connect gate="-F" pin="IOF14" pad="133"/>
<connect gate="-F" pin="IOF2" pad="50"/>
<connect gate="-F" pin="IOF3" pad="51"/>
<connect gate="-F" pin="IOF4" pad="53"/>
<connect gate="-F" pin="IOF5" pad="54"/>
<connect gate="-F" pin="IOF6" pad="55"/>
<connect gate="-F" pin="IOF7" pad="56"/>
<connect gate="-F" pin="IOF8" pad="126"/>
<connect gate="-F" pin="IOF9" pad="127"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="10" pin="VCC" pad="112"/>
<connect gate="11" pin="VCC" pad="122"/>
<connect gate="12" pin="VCC" pad="130"/>
<connect gate="13" pin="VCC" pad="140"/>
<connect gate="14" pin="VCC" pad="150"/>
<connect gate="15" pin="VCC" pad="160"/>
<connect gate="16" pin="VCC" pad="170"/>
<connect gate="17" pin="VCC" pad="189"/>
<connect gate="18" pin="VCC" pad="205"/>
<connect gate="19" pin="VCC" pad="224"/>
<connect gate="2" pin="VCC" pad="16"/>
<connect gate="20" pin="GND" pad="10"/>
<connect gate="21" pin="GND" pad="22"/>
<connect gate="22" pin="GND" pad="32"/>
<connect gate="23" pin="GND" pad="42"/>
<connect gate="24" pin="GND" pad="52"/>
<connect gate="25" pin="GND" pad="69"/>
<connect gate="26" pin="GND" pad="85"/>
<connect gate="27" pin="GND" pad="93"/>
<connect gate="28" pin="GND" pad="104"/>
<connect gate="29" pin="GND" pad="125"/>
<connect gate="3" pin="VCC" pad="27"/>
<connect gate="30" pin="GND" pad="135"/>
<connect gate="31" pin="GND" pad="145"/>
<connect gate="32" pin="GND" pad="155"/>
<connect gate="33" pin="GND" pad="165"/>
<connect gate="34" pin="GND" pad="176"/>
<connect gate="35" pin="GND" pad="197"/>
<connect gate="36" pin="GND" pad="216"/>
<connect gate="37" pin="GND" pad="232"/>
<connect gate="4" pin="VCC" pad="37"/>
<connect gate="5" pin="VCC" pad="47"/>
<connect gate="6" pin="VCC" pad="57"/>
<connect gate="7" pin="VCC" pad="77"/>
<connect gate="8" pin="VCC" pad="89"/>
<connect gate="9" pin="VCC" pad="96"/>
<connect gate="_" pin="/CE" pad="178"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="121"/>
<connect gate="_" pin="/STATUS" pad="60"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="180"/>
<connect gate="_" pin="DCLK" pad="179"/>
<connect gate="_" pin="GCLK0" pad="91"/>
<connect gate="_" pin="GCLK1" pad="211"/>
<connect gate="_" pin="IN0" pad="90"/>
<connect gate="_" pin="IN1" pad="92"/>
<connect gate="_" pin="IN2" pad="210"/>
<connect gate="_" pin="IN3" pad="212"/>
<connect gate="_" pin="MSEL0" pad="124"/>
<connect gate="_" pin="MSEL1" pad="123"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="177"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="58"/>
<connect gate="_" pin="TRST" pad="59"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30AQC240-3N"/>
<attribute name="OC_FARNELL" value="1549384"/>
<attribute name="OC_NEWARK" value="51R8956"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30*-P208" prefix="IC">
<description>&lt;b&gt;EPF10K30&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A9"/>
<gate name="-B" symbol="B10"/>
<gate name="-C" symbol="C11"/>
<gate name="-D" symbol="D11"/>
<gate name="-E" symbol="E10"/>
<gate name="-F" symbol="F10"/>
<gate name="-1" symbol="72-30E"/>
<gate name="-2" symbol="143-30E"/>
<gate name="-3" symbol="221-30E"/>
<gate name="-4" symbol="291-30E"/>
<gate name="-5" symbol="362-30E"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="19" symbol="VCCIO"/>
<gate name="20" symbol="VCCIO"/>
<gate name="21" symbol="VCCIO"/>
<gate name="22" symbol="VCCIO"/>
<gate name="23" symbol="VCCIO"/>
<gate name="24" symbol="VCCIO"/>
<gate name="25" symbol="VCCIO"/>
<gate name="26" symbol="VCCIO"/>
<gate name="27" symbol="GND"/>
<gate name="28" symbol="GND"/>
<gate name="29" symbol="GND"/>
<gate name="30" symbol="GND"/>
<gate name="31" symbol="GND"/>
<gate name="32" symbol="GND"/>
<gate name="33" symbol="GND"/>
<gate name="34" symbol="GND"/>
<gate name="35" symbol="GND"/>
<gate name="36" symbol="GND"/>
<gate name="37" symbol="GND"/>
<gate name="38" symbol="GND"/>
<gate name="39" symbol="GND"/>
<gate name="40" symbol="GND"/>
<gate name="41" symbol="GND"/>
<gate name="42" symbol="GND"/>
<gate name="43" symbol="GND"/>
<gate name="44" symbol="GND"/>
<gate name="45" symbol="GND"/>
<gate name="46" symbol="GND"/>
<gate name="47" symbol="GND"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="-1" pin="IO11" pad="104"/>
<connect gate="-1" pin="IO12" pad="157"/>
<connect gate="-1" pin="IO21" pad="103"/>
<connect gate="-1" pin="IO22" pad="158"/>
<connect gate="-1" pin="IO31" pad="102"/>
<connect gate="-1" pin="IO32" pad="159"/>
<connect gate="-1" pin="IO41" pad="101"/>
<connect gate="-1" pin="IO42" pad="160"/>
<connect gate="-1" pin="IO43" pad="161"/>
<connect gate="-1" pin="IO51" pad="100"/>
<connect gate="-1" pin="IO52" pad="162"/>
<connect gate="-1" pin="IO61" pad="99"/>
<connect gate="-1" pin="IO62" pad="163"/>
<connect gate="-1" pin="IO63" pad="164"/>
<connect gate="-1" pin="IO71" pad="97"/>
<connect gate="-1" pin="IO72" pad="166"/>
<connect gate="-2" pin="IO101" pad="93"/>
<connect gate="-2" pin="IO102" pad="169"/>
<connect gate="-2" pin="IO111" pad="92"/>
<connect gate="-2" pin="IO112" pad="170"/>
<connect gate="-2" pin="IO121" pad="90"/>
<connect gate="-2" pin="IO122" pad="172"/>
<connect gate="-2" pin="IO131" pad="89"/>
<connect gate="-2" pin="IO132" pad="173"/>
<connect gate="-2" pin="IO141" pad="87"/>
<connect gate="-2" pin="IO142" pad="88"/>
<connect gate="-2" pin="IO143" pad="174"/>
<connect gate="-2" pin="IO81" pad="96"/>
<connect gate="-2" pin="IO82" pad="167"/>
<connect gate="-2" pin="IO91" pad="94"/>
<connect gate="-2" pin="IO92" pad="95"/>
<connect gate="-2" pin="IO93" pad="168"/>
<connect gate="-3" pin="IO144" pad="175"/>
<connect gate="-3" pin="IO151" pad="86"/>
<connect gate="-3" pin="IO152" pad="176"/>
<connect gate="-3" pin="IO161" pad="85"/>
<connect gate="-3" pin="IO162" pad="177"/>
<connect gate="-3" pin="IO171" pad="83"/>
<connect gate="-3" pin="IO172" pad="179"/>
<connect gate="-3" pin="IO181" pad="180"/>
<connect gate="-3" pin="IO191" pad="75"/>
<connect gate="-3" pin="IO192" pad="186"/>
<connect gate="-3" pin="IO201" pad="73"/>
<connect gate="-3" pin="IO202" pad="74"/>
<connect gate="-3" pin="IO203" pad="187"/>
<connect gate="-3" pin="IO211" pad="71"/>
<connect gate="-3" pin="IO212" pad="189"/>
<connect gate="-3" pin="IO221" pad="70"/>
<connect gate="-4" pin="IO222" pad="190"/>
<connect gate="-4" pin="IO231" pad="69"/>
<connect gate="-4" pin="IO232" pad="191"/>
<connect gate="-4" pin="IO241" pad="68"/>
<connect gate="-4" pin="IO242" pad="192"/>
<connect gate="-4" pin="IO251" pad="67"/>
<connect gate="-4" pin="IO252" pad="193"/>
<connect gate="-4" pin="IO261" pad="64"/>
<connect gate="-4" pin="IO262" pad="65"/>
<connect gate="-4" pin="IO263" pad="195"/>
<connect gate="-4" pin="IO271" pad="63"/>
<connect gate="-4" pin="IO272" pad="196"/>
<connect gate="-4" pin="IO281" pad="62"/>
<connect gate="-4" pin="IO282" pad="197"/>
<connect gate="-4" pin="IO283" pad="198"/>
<connect gate="-4" pin="IO291" pad="61"/>
<connect gate="-5" pin="IO292" pad="199"/>
<connect gate="-5" pin="IO301" pad="60"/>
<connect gate="-5" pin="IO302" pad="200"/>
<connect gate="-5" pin="IO311" pad="58"/>
<connect gate="-5" pin="IO312" pad="202"/>
<connect gate="-5" pin="IO321" pad="57"/>
<connect gate="-5" pin="IO322" pad="203"/>
<connect gate="-5" pin="IO331" pad="56"/>
<connect gate="-5" pin="IO332" pad="204"/>
<connect gate="-5" pin="IO341" pad="55"/>
<connect gate="-5" pin="IO342" pad="205"/>
<connect gate="-5" pin="IO343" pad="206"/>
<connect gate="-5" pin="IO351" pad="54"/>
<connect gate="-5" pin="IO352" pad="207"/>
<connect gate="-5" pin="IO361" pad="53"/>
<connect gate="-5" pin="IO362" pad="208"/>
<connect gate="-A" pin="IOA1" pad="7"/>
<connect gate="-A" pin="IOA2" pad="8"/>
<connect gate="-A" pin="IOA3" pad="9"/>
<connect gate="-A" pin="IOA4" pad="10"/>
<connect gate="-A" pin="IOA5" pad="11"/>
<connect gate="-A" pin="IOA6" pad="147"/>
<connect gate="-A" pin="IOA7" pad="148"/>
<connect gate="-A" pin="IOA8" pad="149"/>
<connect gate="-A" pin="IOA9" pad="150"/>
<connect gate="-B" pin="IOB1" pad="12"/>
<connect gate="-B" pin="IOB10" pad="144"/>
<connect gate="-B" pin="IOB2" pad="13"/>
<connect gate="-B" pin="IOB3" pad="14"/>
<connect gate="-B" pin="IOB4" pad="15"/>
<connect gate="-B" pin="IOB5" pad="139"/>
<connect gate="-B" pin="IOB6" pad="140"/>
<connect gate="-B" pin="IOB7" pad="141"/>
<connect gate="-B" pin="IOB8" pad="142"/>
<connect gate="-B" pin="IOB9" pad="143"/>
<connect gate="-C" pin="IOC1" pad="16"/>
<connect gate="-C" pin="IOC10" pad="135"/>
<connect gate="-C" pin="IOC11" pad="136"/>
<connect gate="-C" pin="IOC2" pad="17"/>
<connect gate="-C" pin="IOC3" pad="18"/>
<connect gate="-C" pin="IOC4" pad="19"/>
<connect gate="-C" pin="IOC5" pad="24"/>
<connect gate="-C" pin="IOC6" pad="131"/>
<connect gate="-C" pin="IOC7" pad="132"/>
<connect gate="-C" pin="IOC8" pad="133"/>
<connect gate="-C" pin="IOC9" pad="134"/>
<connect gate="-D" pin="IOD1" pad="25"/>
<connect gate="-D" pin="IOD10" pad="127"/>
<connect gate="-D" pin="IOD11" pad="128"/>
<connect gate="-D" pin="IOD2" pad="26"/>
<connect gate="-D" pin="IOD3" pad="27"/>
<connect gate="-D" pin="IOD4" pad="28"/>
<connect gate="-D" pin="IOD5" pad="29"/>
<connect gate="-D" pin="IOD6" pad="30"/>
<connect gate="-D" pin="IOD7" pad="31"/>
<connect gate="-D" pin="IOD8" pad="125"/>
<connect gate="-D" pin="IOD9" pad="126"/>
<connect gate="-E" pin="IOE1" pad="36"/>
<connect gate="-E" pin="IOE10" pad="122"/>
<connect gate="-E" pin="IOE2" pad="37"/>
<connect gate="-E" pin="IOE3" pad="38"/>
<connect gate="-E" pin="IOE4" pad="39"/>
<connect gate="-E" pin="IOE5" pad="40"/>
<connect gate="-E" pin="IOE6" pad="41"/>
<connect gate="-E" pin="IOE7" pad="119"/>
<connect gate="-E" pin="IOE8" pad="120"/>
<connect gate="-E" pin="IOE9" pad="121"/>
<connect gate="-F" pin="IOF1" pad="44"/>
<connect gate="-F" pin="IOF10" pad="116"/>
<connect gate="-F" pin="IOF2" pad="45"/>
<connect gate="-F" pin="IOF3" pad="46"/>
<connect gate="-F" pin="IOF4" pad="47"/>
<connect gate="-F" pin="IOF5" pad="111"/>
<connect gate="-F" pin="IOF6" pad="112"/>
<connect gate="-F" pin="IOF7" pad="113"/>
<connect gate="-F" pin="IOF8" pad="114"/>
<connect gate="-F" pin="IOF9" pad="115"/>
<connect gate="1" pin="VCC" pad="6"/>
<connect gate="10" pin="VCC" pad="137"/>
<connect gate="11" pin="VCC" pad="145"/>
<connect gate="12" pin="VCC" pad="181"/>
<connect gate="13" pin="VCCIO" pad="5"/>
<connect gate="14" pin="VCCIO" pad="22"/>
<connect gate="15" pin="VCCIO" pad="34"/>
<connect gate="16" pin="VCCIO" pad="42"/>
<connect gate="17" pin="VCCIO" pad="66"/>
<connect gate="18" pin="VCCIO" pad="84"/>
<connect gate="19" pin="VCCIO" pad="98"/>
<connect gate="2" pin="VCC" pad="23"/>
<connect gate="20" pin="VCCIO" pad="110"/>
<connect gate="21" pin="VCCIO" pad="118"/>
<connect gate="22" pin="VCCIO" pad="138"/>
<connect gate="23" pin="VCCIO" pad="146"/>
<connect gate="24" pin="VCCIO" pad="165"/>
<connect gate="25" pin="VCCIO" pad="178"/>
<connect gate="26" pin="VCCIO" pad="194"/>
<connect gate="27" pin="GND" pad="20"/>
<connect gate="28" pin="GND" pad="21"/>
<connect gate="29" pin="GND" pad="32"/>
<connect gate="3" pin="VCC" pad="35"/>
<connect gate="30" pin="GND" pad="33"/>
<connect gate="31" pin="GND" pad="48"/>
<connect gate="32" pin="GND" pad="49"/>
<connect gate="33" pin="GND" pad="59"/>
<connect gate="34" pin="GND" pad="72"/>
<connect gate="35" pin="GND" pad="81"/>
<connect gate="36" pin="GND" pad="82"/>
<connect gate="37" pin="GND" pad="91"/>
<connect gate="38" pin="GND" pad="123"/>
<connect gate="39" pin="GND" pad="124"/>
<connect gate="4" pin="VCC" pad="43"/>
<connect gate="40" pin="GND" pad="129"/>
<connect gate="41" pin="GND" pad="130"/>
<connect gate="42" pin="GND" pad="151"/>
<connect gate="43" pin="GND" pad="152"/>
<connect gate="44" pin="GND" pad="171"/>
<connect gate="45" pin="GND" pad="185"/>
<connect gate="46" pin="GND" pad="188"/>
<connect gate="47" pin="GND" pad="201"/>
<connect gate="5" pin="VCC" pad="76"/>
<connect gate="6" pin="VCC" pad="77"/>
<connect gate="7" pin="VCC" pad="106"/>
<connect gate="8" pin="VCC" pad="109"/>
<connect gate="9" pin="VCC" pad="117"/>
<connect gate="_" pin="/CE" pad="154"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="105"/>
<connect gate="_" pin="/STATUS" pad="52"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="156"/>
<connect gate="_" pin="DCLK" pad="155"/>
<connect gate="_" pin="GCLK0" pad="79"/>
<connect gate="_" pin="GCLK1" pad="183"/>
<connect gate="_" pin="IN0" pad="78"/>
<connect gate="_" pin="IN1" pad="80"/>
<connect gate="_" pin="IN2" pad="182"/>
<connect gate="_" pin="IN3" pad="184"/>
<connect gate="_" pin="MSEL0" pad="108"/>
<connect gate="_" pin="MSEL1" pad="107"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="153"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="50"/>
<connect gate="_" pin="TRST" pad="51"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30EQC208-2N"/>
<attribute name="OC_FARNELL" value="1549382"/>
<attribute name="OC_NEWARK" value="51R8987"/>
</technology>
<technology name="A">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30AQI208-3N"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8958"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30-Q208" prefix="IC">
<description>&lt;b&gt;EPF10K30&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A13-30Q"/>
<gate name="-B" symbol="B14-30Q"/>
<gate name="-C" symbol="C14-30Q"/>
<gate name="-D" symbol="D14-30Q"/>
<gate name="-E" symbol="E14-30Q"/>
<gate name="-F" symbol="F14-30Q"/>
<gate name="-1" symbol="37-30Q"/>
<gate name="-2" symbol="143-30Q"/>
<gate name="-3" symbol="221-30Q"/>
<gate name="-4" symbol="292-30Q"/>
<gate name="-5" symbol="363-30Q"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="19" symbol="VCCIO"/>
<gate name="20" symbol="VCCIO"/>
<gate name="21" symbol="VCCIO"/>
<gate name="22" symbol="VCCIO"/>
<gate name="23" symbol="VCCIO"/>
<gate name="24" symbol="VCCIO"/>
<gate name="25" symbol="VCCIO"/>
<gate name="26" symbol="VCCIO"/>
<gate name="27" symbol="GNDINT"/>
<gate name="28" symbol="GNDINT"/>
<gate name="29" symbol="GNDINT"/>
<gate name="30" symbol="GNDINT"/>
<gate name="31" symbol="GNDINT"/>
<gate name="32" symbol="GNDINT"/>
<gate name="33" symbol="GNDINT"/>
<gate name="34" symbol="GNDINT"/>
<gate name="35" symbol="GNDINT"/>
<gate name="36" symbol="GNDIO"/>
<gate name="37" symbol="GNDIO"/>
<gate name="38" symbol="GNDIO"/>
<gate name="39" symbol="GNDIO"/>
<gate name="40" symbol="GNDIO"/>
<gate name="41" symbol="GNDIO"/>
<gate name="42" symbol="GNDIO"/>
<gate name="43" symbol="GNDIO"/>
<gate name="44" symbol="GNDIO"/>
<gate name="45" symbol="GNDIO"/>
<gate name="46" symbol="GNDIO"/>
<gate name="47" symbol="GNDIO"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="-1" pin="IO11" pad="104"/>
<connect gate="-1" pin="IO12" pad="157"/>
<connect gate="-1" pin="IO21" pad="103"/>
<connect gate="-1" pin="IO23" pad="158"/>
<connect gate="-1" pin="IO31" pad="102"/>
<connect gate="-1" pin="IO32" pad="159"/>
<connect gate="-1" pin="IO41" pad="101"/>
<connect gate="-1" pin="IO42" pad="160"/>
<connect gate="-1" pin="IO43" pad="161"/>
<connect gate="-1" pin="IO52" pad="100"/>
<connect gate="-1" pin="IO53" pad="162"/>
<connect gate="-1" pin="IO61" pad="99"/>
<connect gate="-1" pin="IO62" pad="163"/>
<connect gate="-1" pin="IO63" pad="164"/>
<connect gate="-1" pin="IO71" pad="97"/>
<connect gate="-1" pin="IO73" pad="166"/>
<connect gate="-2" pin="IO101" pad="93"/>
<connect gate="-2" pin="IO102" pad="169"/>
<connect gate="-2" pin="IO111" pad="92"/>
<connect gate="-2" pin="IO113" pad="170"/>
<connect gate="-2" pin="IO121" pad="90"/>
<connect gate="-2" pin="IO123" pad="172"/>
<connect gate="-2" pin="IO131" pad="89"/>
<connect gate="-2" pin="IO133" pad="173"/>
<connect gate="-2" pin="IO141" pad="87"/>
<connect gate="-2" pin="IO142" pad="174"/>
<connect gate="-2" pin="IO143" pad="175"/>
<connect gate="-2" pin="IO81" pad="96"/>
<connect gate="-2" pin="IO83" pad="167"/>
<connect gate="-2" pin="IO91" pad="94"/>
<connect gate="-2" pin="IO92" pad="95"/>
<connect gate="-2" pin="IO93" pad="168"/>
<connect gate="-3" pin="IO144" pad="88"/>
<connect gate="-3" pin="IO151" pad="86"/>
<connect gate="-3" pin="IO153" pad="176"/>
<connect gate="-3" pin="IO161" pad="85"/>
<connect gate="-3" pin="IO162" pad="177"/>
<connect gate="-3" pin="IO171" pad="83"/>
<connect gate="-3" pin="IO173" pad="179"/>
<connect gate="-3" pin="IO183" pad="180"/>
<connect gate="-3" pin="IO191" pad="75"/>
<connect gate="-3" pin="IO193" pad="186"/>
<connect gate="-3" pin="IO201" pad="73"/>
<connect gate="-3" pin="IO203" pad="187"/>
<connect gate="-3" pin="IO204" pad="74"/>
<connect gate="-3" pin="IO211" pad="71"/>
<connect gate="-3" pin="IO213" pad="189"/>
<connect gate="-3" pin="IO221" pad="70"/>
<connect gate="-4" pin="IO223" pad="190"/>
<connect gate="-4" pin="IO231" pad="69"/>
<connect gate="-4" pin="IO233" pad="191"/>
<connect gate="-4" pin="IO241" pad="68"/>
<connect gate="-4" pin="IO242" pad="192"/>
<connect gate="-4" pin="IO251" pad="67"/>
<connect gate="-4" pin="IO253" pad="193"/>
<connect gate="-4" pin="IO261" pad="64"/>
<connect gate="-4" pin="IO262" pad="65"/>
<connect gate="-4" pin="IO263" pad="195"/>
<connect gate="-4" pin="IO271" pad="63"/>
<connect gate="-4" pin="IO273" pad="196"/>
<connect gate="-4" pin="IO281" pad="62"/>
<connect gate="-4" pin="IO282" pad="198"/>
<connect gate="-4" pin="IO284" pad="197"/>
<connect gate="-4" pin="IO292" pad="61"/>
<connect gate="-5" pin="IO293" pad="199"/>
<connect gate="-5" pin="IO301" pad="60"/>
<connect gate="-5" pin="IO303" pad="200"/>
<connect gate="-5" pin="IO311" pad="58"/>
<connect gate="-5" pin="IO313" pad="202"/>
<connect gate="-5" pin="IO321" pad="57"/>
<connect gate="-5" pin="IO323" pad="203"/>
<connect gate="-5" pin="IO331" pad="56"/>
<connect gate="-5" pin="IO332" pad="204"/>
<connect gate="-5" pin="IO341" pad="55"/>
<connect gate="-5" pin="IO342" pad="205"/>
<connect gate="-5" pin="IO343" pad="206"/>
<connect gate="-5" pin="IO351" pad="54"/>
<connect gate="-5" pin="IO352" pad="207"/>
<connect gate="-5" pin="IO361" pad="53"/>
<connect gate="-5" pin="IO363" pad="208"/>
<connect gate="-A" pin="IOA1" pad="7"/>
<connect gate="-A" pin="IOA12" pad="149"/>
<connect gate="-A" pin="IOA13" pad="150"/>
<connect gate="-A" pin="IOA3" pad="8"/>
<connect gate="-A" pin="IOA4" pad="9"/>
<connect gate="-A" pin="IOA5" pad="10"/>
<connect gate="-A" pin="IOA7" pad="11"/>
<connect gate="-A" pin="IOA8" pad="147"/>
<connect gate="-A" pin="IOA9" pad="148"/>
<connect gate="-B" pin="IOB10" pad="141"/>
<connect gate="-B" pin="IOB11" pad="142"/>
<connect gate="-B" pin="IOB12" pad="143"/>
<connect gate="-B" pin="IOB14" pad="144"/>
<connect gate="-B" pin="IOB2" pad="12"/>
<connect gate="-B" pin="IOB3" pad="13"/>
<connect gate="-B" pin="IOB5" pad="14"/>
<connect gate="-B" pin="IOB7" pad="15"/>
<connect gate="-B" pin="IOB8" pad="139"/>
<connect gate="-B" pin="IOB9" pad="140"/>
<connect gate="-C" pin="IOC1" pad="16"/>
<connect gate="-C" pin="IOC10" pad="133"/>
<connect gate="-C" pin="IOC11" pad="134"/>
<connect gate="-C" pin="IOC12" pad="135"/>
<connect gate="-C" pin="IOC14" pad="136"/>
<connect gate="-C" pin="IOC2" pad="17"/>
<connect gate="-C" pin="IOC3" pad="18"/>
<connect gate="-C" pin="IOC4" pad="19"/>
<connect gate="-C" pin="IOC7" pad="24"/>
<connect gate="-C" pin="IOC8" pad="131"/>
<connect gate="-C" pin="IOC9" pad="132"/>
<connect gate="-D" pin="IOD1" pad="25"/>
<connect gate="-D" pin="IOD10" pad="126"/>
<connect gate="-D" pin="IOD12" pad="127"/>
<connect gate="-D" pin="IOD14" pad="128"/>
<connect gate="-D" pin="IOD2" pad="26"/>
<connect gate="-D" pin="IOD3" pad="27"/>
<connect gate="-D" pin="IOD4" pad="28"/>
<connect gate="-D" pin="IOD5" pad="29"/>
<connect gate="-D" pin="IOD6" pad="30"/>
<connect gate="-D" pin="IOD7" pad="31"/>
<connect gate="-D" pin="IOD8" pad="125"/>
<connect gate="-E" pin="IOE1" pad="36"/>
<connect gate="-E" pin="IOE10" pad="120"/>
<connect gate="-E" pin="IOE12" pad="121"/>
<connect gate="-E" pin="IOE14" pad="122"/>
<connect gate="-E" pin="IOE3" pad="37"/>
<connect gate="-E" pin="IOE4" pad="38"/>
<connect gate="-E" pin="IOE5" pad="39"/>
<connect gate="-E" pin="IOE6" pad="40"/>
<connect gate="-E" pin="IOE7" pad="41"/>
<connect gate="-E" pin="IOE8" pad="119"/>
<connect gate="-F" pin="IOF1" pad="44"/>
<connect gate="-F" pin="IOF10" pad="113"/>
<connect gate="-F" pin="IOF11" pad="114"/>
<connect gate="-F" pin="IOF12" pad="115"/>
<connect gate="-F" pin="IOF14" pad="116"/>
<connect gate="-F" pin="IOF3" pad="45"/>
<connect gate="-F" pin="IOF5" pad="46"/>
<connect gate="-F" pin="IOF7" pad="47"/>
<connect gate="-F" pin="IOF8" pad="111"/>
<connect gate="-F" pin="IOF9" pad="112"/>
<connect gate="1" pin="VCC" pad="6"/>
<connect gate="10" pin="VCC" pad="137"/>
<connect gate="11" pin="VCC" pad="145"/>
<connect gate="12" pin="VCC" pad="181"/>
<connect gate="13" pin="VCCIO" pad="5"/>
<connect gate="14" pin="VCCIO" pad="22"/>
<connect gate="15" pin="VCCIO" pad="34"/>
<connect gate="16" pin="VCCIO" pad="42"/>
<connect gate="17" pin="VCCIO" pad="66"/>
<connect gate="18" pin="VCCIO" pad="84"/>
<connect gate="19" pin="VCCIO" pad="98"/>
<connect gate="2" pin="VCC" pad="23"/>
<connect gate="20" pin="VCCIO" pad="110"/>
<connect gate="21" pin="VCCIO" pad="118"/>
<connect gate="22" pin="VCCIO" pad="138"/>
<connect gate="23" pin="VCCIO" pad="146"/>
<connect gate="24" pin="VCCIO" pad="165"/>
<connect gate="25" pin="VCCIO" pad="178"/>
<connect gate="26" pin="VCCIO" pad="194"/>
<connect gate="27" pin="GND" pad="21"/>
<connect gate="28" pin="GND" pad="33"/>
<connect gate="29" pin="GND" pad="49"/>
<connect gate="3" pin="VCC" pad="35"/>
<connect gate="30" pin="GND" pad="81"/>
<connect gate="31" pin="GND" pad="82"/>
<connect gate="32" pin="GND" pad="123"/>
<connect gate="33" pin="GND" pad="129"/>
<connect gate="34" pin="GND" pad="151"/>
<connect gate="35" pin="GND" pad="185"/>
<connect gate="36" pin="GNDIO" pad="20"/>
<connect gate="37" pin="GNDIO" pad="32"/>
<connect gate="38" pin="GNDIO" pad="48"/>
<connect gate="39" pin="GNDIO" pad="59"/>
<connect gate="4" pin="VCC" pad="43"/>
<connect gate="40" pin="GNDIO" pad="72"/>
<connect gate="41" pin="GNDIO" pad="91"/>
<connect gate="42" pin="GNDIO" pad="124"/>
<connect gate="43" pin="GNDIO" pad="130"/>
<connect gate="44" pin="GNDIO" pad="152"/>
<connect gate="45" pin="GNDIO" pad="171"/>
<connect gate="46" pin="GNDIO" pad="188"/>
<connect gate="47" pin="GNDIO" pad="201"/>
<connect gate="5" pin="VCC" pad="76"/>
<connect gate="6" pin="VCC" pad="77"/>
<connect gate="7" pin="VCC" pad="106"/>
<connect gate="8" pin="VCC" pad="109"/>
<connect gate="9" pin="VCC" pad="117"/>
<connect gate="_" pin="/CE" pad="154"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="105"/>
<connect gate="_" pin="/STATUS" pad="52"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="156"/>
<connect gate="_" pin="DCLK" pad="155"/>
<connect gate="_" pin="GCLK0" pad="79"/>
<connect gate="_" pin="GCLK1" pad="183"/>
<connect gate="_" pin="IN0" pad="78"/>
<connect gate="_" pin="IN1" pad="80"/>
<connect gate="_" pin="IN2" pad="182"/>
<connect gate="_" pin="IN3" pad="184"/>
<connect gate="_" pin="MSEL0" pad="108"/>
<connect gate="_" pin="MSEL1" pad="107"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="153"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="50"/>
<connect gate="_" pin="TRST" pad="51"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30EQC208-2N"/>
<attribute name="OC_FARNELL" value="1549382"/>
<attribute name="OC_NEWARK" value="51R8987"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K20-R240" prefix="IC">
<description>&lt;b&gt;EPF10K20&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A16-15"/>
<gate name="-B" symbol="B16-15"/>
<gate name="-C" symbol="C16-14"/>
<gate name="-D" symbol="D15-14"/>
<gate name="-E" symbol="E15-14"/>
<gate name="-F" symbol="F15"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCINT"/>
<gate name="14" symbol="VCCINT"/>
<gate name="15" symbol="VCCINT"/>
<gate name="16" symbol="VCCINT"/>
<gate name="17" symbol="VCCINT"/>
<gate name="18" symbol="VCCINT"/>
<gate name="19" symbol="VCCINT"/>
<gate name="20" symbol="GNDINT"/>
<gate name="21" symbol="GNDINT"/>
<gate name="22" symbol="GNDINT"/>
<gate name="23" symbol="GNDINT"/>
<gate name="24" symbol="GNDINT"/>
<gate name="25" symbol="GNDINT"/>
<gate name="26" symbol="GNDINT"/>
<gate name="27" symbol="GNDINT"/>
<gate name="28" symbol="GNDINT"/>
<gate name="29" symbol="GNDINT"/>
<gate name="30" symbol="GNDINT"/>
<gate name="31" symbol="GNDINT"/>
<gate name="32" symbol="GNDINT"/>
<gate name="33" symbol="GNDINT"/>
<gate name="34" symbol="GNDINT"/>
<gate name="35" symbol="GNDINT"/>
<gate name="36" symbol="GNDINT"/>
<gate name="37" symbol="GNDINT"/>
</gates>
<devices>
<device name="" package="RQFP240">
<connects>
<connect gate="-1" pin="IO11" pad="120"/>
<connect gate="-1" pin="IO12" pad="182"/>
<connect gate="-1" pin="IO13" pad="183"/>
<connect gate="-1" pin="IO14" pad="119"/>
<connect gate="-1" pin="IO21" pad="117"/>
<connect gate="-1" pin="IO22" pad="118"/>
<connect gate="-1" pin="IO23" pad="184"/>
<connect gate="-1" pin="IO24" pad="185"/>
<connect gate="-1" pin="IO31" pad="116"/>
<connect gate="-1" pin="IO32" pad="186"/>
<connect gate="-1" pin="IO33" pad="187"/>
<connect gate="-1" pin="IO34" pad="115"/>
<connect gate="-1" pin="IO41" pad="113"/>
<connect gate="-1" pin="IO42" pad="114"/>
<connect gate="-1" pin="IO43" pad="188"/>
<connect gate="-1" pin="IO44" pad="190"/>
<connect gate="-2" pin="IO51" pad="110"/>
<connect gate="-2" pin="IO52" pad="111"/>
<connect gate="-2" pin="IO53" pad="191"/>
<connect gate="-2" pin="IO54" pad="192"/>
<connect gate="-2" pin="IO61" pad="109"/>
<connect gate="-2" pin="IO62" pad="193"/>
<connect gate="-2" pin="IO63" pad="194"/>
<connect gate="-2" pin="IO64" pad="108"/>
<connect gate="-2" pin="IO71" pad="106"/>
<connect gate="-2" pin="IO72" pad="107"/>
<connect gate="-2" pin="IO73" pad="195"/>
<connect gate="-2" pin="IO74" pad="196"/>
<connect gate="-2" pin="IO81" pad="103"/>
<connect gate="-2" pin="IO82" pad="105"/>
<connect gate="-2" pin="IO83" pad="198"/>
<connect gate="-2" pin="IO84" pad="199"/>
<connect gate="-3" pin="IO101" pad="100"/>
<connect gate="-3" pin="IO102" pad="202"/>
<connect gate="-3" pin="IO103" pad="203"/>
<connect gate="-3" pin="IO104" pad="99"/>
<connect gate="-3" pin="IO111" pad="97"/>
<connect gate="-3" pin="IO112" pad="98"/>
<connect gate="-3" pin="IO113" pad="204"/>
<connect gate="-3" pin="IO114" pad="206"/>
<connect gate="-3" pin="IO121" pad="95"/>
<connect gate="-3" pin="IO122" pad="207"/>
<connect gate="-3" pin="IO123" pad="94"/>
<connect gate="-3" pin="IO124" pad="208"/>
<connect gate="-3" pin="IO91" pad="101"/>
<connect gate="-3" pin="IO92" pad="102"/>
<connect gate="-3" pin="IO93" pad="200"/>
<connect gate="-3" pin="IO94" pad="201"/>
<connect gate="-4" pin="IO131" pad="87"/>
<connect gate="-4" pin="IO132" pad="88"/>
<connect gate="-4" pin="IO133" pad="209"/>
<connect gate="-4" pin="IO134" pad="213"/>
<connect gate="-4" pin="IO141" pad="84"/>
<connect gate="-4" pin="IO142" pad="86"/>
<connect gate="-4" pin="IO143" pad="214"/>
<connect gate="-4" pin="IO144" pad="215"/>
<connect gate="-4" pin="IO151" pad="82"/>
<connect gate="-4" pin="IO152" pad="83"/>
<connect gate="-4" pin="IO153" pad="218"/>
<connect gate="-4" pin="IO154" pad="217"/>
<connect gate="-4" pin="IO161" pad="81"/>
<connect gate="-4" pin="IO162" pad="219"/>
<connect gate="-4" pin="IO163" pad="220"/>
<connect gate="-4" pin="IO164" pad="80"/>
<connect gate="-5" pin="IO171" pad="79"/>
<connect gate="-5" pin="IO172" pad="222"/>
<connect gate="-5" pin="IO173" pad="221"/>
<connect gate="-5" pin="IO174" pad="78"/>
<connect gate="-5" pin="IO181" pad="75"/>
<connect gate="-5" pin="IO182" pad="76"/>
<connect gate="-5" pin="IO183" pad="223"/>
<connect gate="-5" pin="IO184" pad="225"/>
<connect gate="-5" pin="IO191" pad="73"/>
<connect gate="-5" pin="IO192" pad="74"/>
<connect gate="-5" pin="IO193" pad="227"/>
<connect gate="-5" pin="IO194" pad="226"/>
<connect gate="-5" pin="IO201" pad="71"/>
<connect gate="-5" pin="IO202" pad="228"/>
<connect gate="-5" pin="IO203" pad="229"/>
<connect gate="-5" pin="IO204" pad="72"/>
<connect gate="-6" pin="IO211" pad="68"/>
<connect gate="-6" pin="IO212" pad="70"/>
<connect gate="-6" pin="IO213" pad="230"/>
<connect gate="-6" pin="IO214" pad="231"/>
<connect gate="-6" pin="IO221" pad="66"/>
<connect gate="-6" pin="IO222" pad="234"/>
<connect gate="-6" pin="IO223" pad="67"/>
<connect gate="-6" pin="IO224" pad="233"/>
<connect gate="-6" pin="IO231" pad="64"/>
<connect gate="-6" pin="IO232" pad="236"/>
<connect gate="-6" pin="IO233" pad="235"/>
<connect gate="-6" pin="IO234" pad="65"/>
<connect gate="-6" pin="IO241" pad="62"/>
<connect gate="-6" pin="IO242" pad="63"/>
<connect gate="-6" pin="IO243" pad="237"/>
<connect gate="-6" pin="IO244" pad="238"/>
<connect gate="-A" pin="IOA1" pad="6"/>
<connect gate="-A" pin="IOA10" pad="239"/>
<connect gate="-A" pin="IOA11" pad="240"/>
<connect gate="-A" pin="IOA12" pad="12"/>
<connect gate="-A" pin="IOA13" pad="174"/>
<connect gate="-A" pin="IOA14" pad="172"/>
<connect gate="-A" pin="IOA15" pad="8"/>
<connect gate="-A" pin="IOA16" pad="169"/>
<connect gate="-A" pin="IOA2" pad="7"/>
<connect gate="-A" pin="IOA3" pad="9"/>
<connect gate="-A" pin="IOA4" pad="11"/>
<connect gate="-A" pin="IOA6" pad="171"/>
<connect gate="-A" pin="IOA7" pad="173"/>
<connect gate="-A" pin="IOA8" pad="175"/>
<connect gate="-A" pin="IOA9" pad="181"/>
<connect gate="-B" pin="IOB1" pad="13"/>
<connect gate="-B" pin="IOB10" pad="166"/>
<connect gate="-B" pin="IOB11" pad="168"/>
<connect gate="-B" pin="IOB12" pad="167"/>
<connect gate="-B" pin="IOB13" pad="14"/>
<connect gate="-B" pin="IOB14" pad="15"/>
<connect gate="-B" pin="IOB15" pad="19"/>
<connect gate="-B" pin="IOB2" pad="17"/>
<connect gate="-B" pin="IOB3" pad="18"/>
<connect gate="-B" pin="IOB4" pad="20"/>
<connect gate="-B" pin="IOB5" pad="21"/>
<connect gate="-B" pin="IOB6" pad="161"/>
<connect gate="-B" pin="IOB7" pad="162"/>
<connect gate="-B" pin="IOB8" pad="163"/>
<connect gate="-B" pin="IOB9" pad="164"/>
<connect gate="-C" pin="IOC1" pad="23"/>
<connect gate="-C" pin="IOC10" pad="159"/>
<connect gate="-C" pin="IOC12" pad="158"/>
<connect gate="-C" pin="IOC13" pad="25"/>
<connect gate="-C" pin="IOC14" pad="28"/>
<connect gate="-C" pin="IOC15" pad="29"/>
<connect gate="-C" pin="IOC16" pad="30"/>
<connect gate="-C" pin="IOC3" pad="24"/>
<connect gate="-C" pin="IOC4" pad="26"/>
<connect gate="-C" pin="IOC5" pad="152"/>
<connect gate="-C" pin="IOC6" pad="153"/>
<connect gate="-C" pin="IOC7" pad="154"/>
<connect gate="-C" pin="IOC8" pad="156"/>
<connect gate="-C" pin="IOC9" pad="157"/>
<connect gate="-D" pin="IOD1" pad="31"/>
<connect gate="-D" pin="IOD10" pad="147"/>
<connect gate="-D" pin="IOD11" pad="151"/>
<connect gate="-D" pin="IOD12" pad="144"/>
<connect gate="-D" pin="IOD13" pad="146"/>
<connect gate="-D" pin="IOD14" pad="149"/>
<connect gate="-D" pin="IOD15" pad="148"/>
<connect gate="-D" pin="IOD3" pad="33"/>
<connect gate="-D" pin="IOD4" pad="34"/>
<connect gate="-D" pin="IOD5" pad="35"/>
<connect gate="-D" pin="IOD6" pad="36"/>
<connect gate="-D" pin="IOD7" pad="38"/>
<connect gate="-D" pin="IOD8" pad="39"/>
<connect gate="-D" pin="IOD9" pad="143"/>
<connect gate="-E" pin="IOE1" pad="40"/>
<connect gate="-E" pin="IOE10" pad="137"/>
<connect gate="-E" pin="IOE11" pad="141"/>
<connect gate="-E" pin="IOE12" pad="139"/>
<connect gate="-E" pin="IOE13" pad="142"/>
<connect gate="-E" pin="IOE14" pad="138"/>
<connect gate="-E" pin="IOE15" pad="46"/>
<connect gate="-E" pin="IOE2" pad="41"/>
<connect gate="-E" pin="IOE3" pad="43"/>
<connect gate="-E" pin="IOE4" pad="44"/>
<connect gate="-E" pin="IOE5" pad="45"/>
<connect gate="-E" pin="IOE6" pad="48"/>
<connect gate="-E" pin="IOE8" pad="134"/>
<connect gate="-E" pin="IOE9" pad="136"/>
<connect gate="-F" pin="IOF1" pad="49"/>
<connect gate="-F" pin="IOF10" pad="131"/>
<connect gate="-F" pin="IOF11" pad="133"/>
<connect gate="-F" pin="IOF12" pad="51"/>
<connect gate="-F" pin="IOF13" pad="132"/>
<connect gate="-F" pin="IOF14" pad="53"/>
<connect gate="-F" pin="IOF15" pad="56"/>
<connect gate="-F" pin="IOF2" pad="50"/>
<connect gate="-F" pin="IOF3" pad="54"/>
<connect gate="-F" pin="IOF4" pad="55"/>
<connect gate="-F" pin="IOF5" pad="61"/>
<connect gate="-F" pin="IOF6" pad="126"/>
<connect gate="-F" pin="IOF7" pad="127"/>
<connect gate="-F" pin="IOF8" pad="128"/>
<connect gate="-F" pin="IOF9" pad="129"/>
<connect gate="1" pin="VCC" pad="5"/>
<connect gate="10" pin="VCC" pad="112"/>
<connect gate="11" pin="VCC" pad="122"/>
<connect gate="12" pin="VCC" pad="130"/>
<connect gate="13" pin="VCC" pad="140"/>
<connect gate="14" pin="VCC" pad="150"/>
<connect gate="15" pin="VCC" pad="160"/>
<connect gate="16" pin="VCC" pad="170"/>
<connect gate="17" pin="VCC" pad="189"/>
<connect gate="18" pin="VCC" pad="205"/>
<connect gate="19" pin="VCC" pad="224"/>
<connect gate="2" pin="VCC" pad="16"/>
<connect gate="20" pin="GND" pad="10"/>
<connect gate="21" pin="GND" pad="22"/>
<connect gate="22" pin="GND" pad="32"/>
<connect gate="23" pin="GND" pad="42"/>
<connect gate="24" pin="GND" pad="52"/>
<connect gate="25" pin="GND" pad="69"/>
<connect gate="26" pin="GND" pad="85"/>
<connect gate="27" pin="GND" pad="93"/>
<connect gate="28" pin="GND" pad="104"/>
<connect gate="29" pin="GND" pad="125"/>
<connect gate="3" pin="VCC" pad="27"/>
<connect gate="30" pin="GND" pad="135"/>
<connect gate="31" pin="GND" pad="145"/>
<connect gate="32" pin="GND" pad="155"/>
<connect gate="33" pin="GND" pad="165"/>
<connect gate="34" pin="GND" pad="176"/>
<connect gate="35" pin="GND" pad="197"/>
<connect gate="36" pin="GND" pad="216"/>
<connect gate="37" pin="GND" pad="232"/>
<connect gate="4" pin="VCC" pad="37"/>
<connect gate="5" pin="VCC" pad="47"/>
<connect gate="6" pin="VCC" pad="57"/>
<connect gate="7" pin="VCC" pad="77"/>
<connect gate="8" pin="VCC" pad="89"/>
<connect gate="9" pin="VCC" pad="96"/>
<connect gate="_" pin="/CE" pad="178"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="121"/>
<connect gate="_" pin="/STATUS" pad="60"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="180"/>
<connect gate="_" pin="DCLK" pad="179"/>
<connect gate="_" pin="GCLK0" pad="91"/>
<connect gate="_" pin="GCLK1" pad="211"/>
<connect gate="_" pin="IN0" pad="90"/>
<connect gate="_" pin="IN1" pad="92"/>
<connect gate="_" pin="IN2" pad="210"/>
<connect gate="_" pin="IN3" pad="212"/>
<connect gate="_" pin="MSEL0" pad="124"/>
<connect gate="_" pin="MSEL1" pad="123"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="177"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="58"/>
<connect gate="_" pin="TRST" pad="59"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K20RC240-3N"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8884"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K20-R208" prefix="IC">
<description>&lt;b&gt;EPF10K20&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A11"/>
<gate name="-B" symbol="B11"/>
<gate name="-C" symbol="C10"/>
<gate name="-D" symbol="D11"/>
<gate name="-E" symbol="E11"/>
<gate name="-F" symbol="F11"/>
<gate name="-1" symbol="52-20R"/>
<gate name="-2" symbol="102-20R"/>
<gate name="-3" symbol="152-20R"/>
<gate name="-4" symbol="203-20R"/>
<gate name="-5" symbol="244-20R"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="19" symbol="VCCIO"/>
<gate name="20" symbol="VCCIO"/>
<gate name="21" symbol="VCCIO"/>
<gate name="22" symbol="VCCIO"/>
<gate name="23" symbol="VCCIO"/>
<gate name="24" symbol="VCCIO"/>
<gate name="25" symbol="VCCIO"/>
<gate name="26" symbol="VCCIO"/>
<gate name="27" symbol="GNDINT"/>
<gate name="28" symbol="GNDINT"/>
<gate name="29" symbol="GNDINT"/>
<gate name="30" symbol="GNDINT"/>
<gate name="31" symbol="GNDINT"/>
<gate name="32" symbol="GNDINT"/>
<gate name="33" symbol="GNDINT"/>
<gate name="34" symbol="GNDINT"/>
<gate name="35" symbol="GNDINT"/>
<gate name="36" symbol="GNDIO"/>
<gate name="37" symbol="GNDIO"/>
<gate name="38" symbol="GNDIO"/>
<gate name="39" symbol="GNDIO"/>
<gate name="40" symbol="GNDIO"/>
<gate name="41" symbol="GNDIO"/>
<gate name="42" symbol="GNDIO"/>
<gate name="43" symbol="GNDIO"/>
<gate name="44" symbol="GNDIO"/>
<gate name="45" symbol="GNDIO"/>
<gate name="46" symbol="GNDIO"/>
<gate name="47" symbol="GNDIO"/>
</gates>
<devices>
<device name="" package="RQFP208">
<connects>
<connect gate="-1" pin="IO11" pad="104"/>
<connect gate="-1" pin="IO12" pad="158"/>
<connect gate="-1" pin="IO13" pad="159"/>
<connect gate="-1" pin="IO21" pad="102"/>
<connect gate="-1" pin="IO22" pad="103"/>
<connect gate="-1" pin="IO23" pad="160"/>
<connect gate="-1" pin="IO24" pad="161"/>
<connect gate="-1" pin="IO31" pad="101"/>
<connect gate="-1" pin="IO32" pad="162"/>
<connect gate="-1" pin="IO33" pad="163"/>
<connect gate="-1" pin="IO41" pad="99"/>
<connect gate="-1" pin="IO42" pad="100"/>
<connect gate="-1" pin="IO43" pad="164"/>
<connect gate="-1" pin="IO44" pad="166"/>
<connect gate="-1" pin="IO51" pad="96"/>
<connect gate="-1" pin="IO52" pad="97"/>
<connect gate="-2" pin="IO101" pad="87"/>
<connect gate="-2" pin="IO102" pad="175"/>
<connect gate="-2" pin="IO53" pad="167"/>
<connect gate="-2" pin="IO61" pad="95"/>
<connect gate="-2" pin="IO62" pad="168"/>
<connect gate="-2" pin="IO63" pad="169"/>
<connect gate="-2" pin="IO71" pad="93"/>
<connect gate="-2" pin="IO72" pad="94"/>
<connect gate="-2" pin="IO73" pad="170"/>
<connect gate="-2" pin="IO81" pad="90"/>
<connect gate="-2" pin="IO82" pad="92"/>
<connect gate="-2" pin="IO83" pad="172"/>
<connect gate="-2" pin="IO91" pad="88"/>
<connect gate="-2" pin="IO92" pad="89"/>
<connect gate="-2" pin="IO93" pad="173"/>
<connect gate="-2" pin="IO94" pad="174"/>
<connect gate="-3" pin="IO111" pad="85"/>
<connect gate="-3" pin="IO112" pad="86"/>
<connect gate="-3" pin="IO113" pad="176"/>
<connect gate="-3" pin="IO114" pad="177"/>
<connect gate="-3" pin="IO121" pad="83"/>
<connect gate="-3" pin="IO122" pad="179"/>
<connect gate="-3" pin="IO131" pad="74"/>
<connect gate="-3" pin="IO132" pad="75"/>
<connect gate="-3" pin="IO133" pad="180"/>
<connect gate="-3" pin="IO134" pad="186"/>
<connect gate="-3" pin="IO141" pad="71"/>
<connect gate="-3" pin="IO142" pad="73"/>
<connect gate="-3" pin="IO143" pad="187"/>
<connect gate="-3" pin="IO144" pad="189"/>
<connect gate="-3" pin="IO151" pad="69"/>
<connect gate="-3" pin="IO152" pad="70"/>
<connect gate="-4" pin="IO153" pad="190"/>
<connect gate="-4" pin="IO161" pad="68"/>
<connect gate="-4" pin="IO162" pad="191"/>
<connect gate="-4" pin="IO163" pad="192"/>
<connect gate="-4" pin="IO171" pad="67"/>
<connect gate="-4" pin="IO172" pad="193"/>
<connect gate="-4" pin="IO181" pad="64"/>
<connect gate="-4" pin="IO182" pad="65"/>
<connect gate="-4" pin="IO183" pad="195"/>
<connect gate="-4" pin="IO184" pad="196"/>
<connect gate="-4" pin="IO191" pad="62"/>
<connect gate="-4" pin="IO192" pad="63"/>
<connect gate="-4" pin="IO193" pad="197"/>
<connect gate="-4" pin="IO201" pad="61"/>
<connect gate="-4" pin="IO202" pad="198"/>
<connect gate="-4" pin="IO203" pad="199"/>
<connect gate="-5" pin="IO211" pad="58"/>
<connect gate="-5" pin="IO212" pad="60"/>
<connect gate="-5" pin="IO213" pad="200"/>
<connect gate="-5" pin="IO214" pad="202"/>
<connect gate="-5" pin="IO221" pad="57"/>
<connect gate="-5" pin="IO222" pad="203"/>
<connect gate="-5" pin="IO231" pad="56"/>
<connect gate="-5" pin="IO232" pad="204"/>
<connect gate="-5" pin="IO241" pad="54"/>
<connect gate="-5" pin="IO242" pad="55"/>
<connect gate="-5" pin="IO243" pad="205"/>
<connect gate="-5" pin="IO244" pad="206"/>
<connect gate="-A" pin="IOA1" pad="7"/>
<connect gate="-A" pin="IOA10" pad="207"/>
<connect gate="-A" pin="IOA11" pad="208"/>
<connect gate="-A" pin="IOA2" pad="8"/>
<connect gate="-A" pin="IOA3" pad="9"/>
<connect gate="-A" pin="IOA4" pad="10"/>
<connect gate="-A" pin="IOA5" pad="147"/>
<connect gate="-A" pin="IOA6" pad="148"/>
<connect gate="-A" pin="IOA7" pad="149"/>
<connect gate="-A" pin="IOA8" pad="150"/>
<connect gate="-A" pin="IOA9" pad="157"/>
<connect gate="-B" pin="IOB1" pad="11"/>
<connect gate="-B" pin="IOB10" pad="143"/>
<connect gate="-B" pin="IOB11" pad="144"/>
<connect gate="-B" pin="IOB2" pad="12"/>
<connect gate="-B" pin="IOB3" pad="13"/>
<connect gate="-B" pin="IOB4" pad="14"/>
<connect gate="-B" pin="IOB5" pad="15"/>
<connect gate="-B" pin="IOB6" pad="139"/>
<connect gate="-B" pin="IOB7" pad="140"/>
<connect gate="-B" pin="IOB8" pad="141"/>
<connect gate="-B" pin="IOB9" pad="142"/>
<connect gate="-C" pin="IOC1" pad="16"/>
<connect gate="-C" pin="IOC10" pad="136"/>
<connect gate="-C" pin="IOC2" pad="17"/>
<connect gate="-C" pin="IOC3" pad="18"/>
<connect gate="-C" pin="IOC4" pad="19"/>
<connect gate="-C" pin="IOC5" pad="131"/>
<connect gate="-C" pin="IOC6" pad="132"/>
<connect gate="-C" pin="IOC7" pad="133"/>
<connect gate="-C" pin="IOC8" pad="134"/>
<connect gate="-C" pin="IOC9" pad="135"/>
<connect gate="-D" pin="IOD1" pad="24"/>
<connect gate="-D" pin="IOD10" pad="127"/>
<connect gate="-D" pin="IOD11" pad="128"/>
<connect gate="-D" pin="IOD2" pad="25"/>
<connect gate="-D" pin="IOD3" pad="26"/>
<connect gate="-D" pin="IOD4" pad="27"/>
<connect gate="-D" pin="IOD5" pad="28"/>
<connect gate="-D" pin="IOD6" pad="29"/>
<connect gate="-D" pin="IOD7" pad="30"/>
<connect gate="-D" pin="IOD8" pad="31"/>
<connect gate="-D" pin="IOD9" pad="126"/>
<connect gate="-E" pin="IOE1" pad="36"/>
<connect gate="-E" pin="IOE10" pad="122"/>
<connect gate="-E" pin="IOE11" pad="125"/>
<connect gate="-E" pin="IOE2" pad="37"/>
<connect gate="-E" pin="IOE3" pad="38"/>
<connect gate="-E" pin="IOE4" pad="39"/>
<connect gate="-E" pin="IOE5" pad="40"/>
<connect gate="-E" pin="IOE6" pad="41"/>
<connect gate="-E" pin="IOE7" pad="119"/>
<connect gate="-E" pin="IOE8" pad="120"/>
<connect gate="-E" pin="IOE9" pad="121"/>
<connect gate="-F" pin="IOF1" pad="44"/>
<connect gate="-F" pin="IOF10" pad="115"/>
<connect gate="-F" pin="IOF11" pad="116"/>
<connect gate="-F" pin="IOF2" pad="45"/>
<connect gate="-F" pin="IOF3" pad="46"/>
<connect gate="-F" pin="IOF4" pad="47"/>
<connect gate="-F" pin="IOF5" pad="53"/>
<connect gate="-F" pin="IOF6" pad="111"/>
<connect gate="-F" pin="IOF7" pad="112"/>
<connect gate="-F" pin="IOF8" pad="113"/>
<connect gate="-F" pin="IOF9" pad="114"/>
<connect gate="1" pin="VCC" pad="6"/>
<connect gate="10" pin="VCC" pad="137"/>
<connect gate="11" pin="VCC" pad="145"/>
<connect gate="12" pin="VCC" pad="181"/>
<connect gate="13" pin="VCCIO" pad="5"/>
<connect gate="14" pin="VCCIO" pad="22"/>
<connect gate="15" pin="VCCIO" pad="34"/>
<connect gate="16" pin="VCCIO" pad="42"/>
<connect gate="17" pin="VCCIO" pad="66"/>
<connect gate="18" pin="VCCIO" pad="84"/>
<connect gate="19" pin="VCCIO" pad="98"/>
<connect gate="2" pin="VCC" pad="23"/>
<connect gate="20" pin="VCCIO" pad="110"/>
<connect gate="21" pin="VCCIO" pad="118"/>
<connect gate="22" pin="VCCIO" pad="138"/>
<connect gate="23" pin="VCCIO" pad="146"/>
<connect gate="24" pin="VCCIO" pad="165"/>
<connect gate="25" pin="VCCIO" pad="178"/>
<connect gate="26" pin="VCCIO" pad="194"/>
<connect gate="27" pin="GND" pad="21"/>
<connect gate="28" pin="GND" pad="33"/>
<connect gate="29" pin="GND" pad="49"/>
<connect gate="3" pin="VCC" pad="35"/>
<connect gate="30" pin="GND" pad="81"/>
<connect gate="31" pin="GND" pad="82"/>
<connect gate="32" pin="GND" pad="123"/>
<connect gate="33" pin="GND" pad="129"/>
<connect gate="34" pin="GND" pad="151"/>
<connect gate="35" pin="GND" pad="185"/>
<connect gate="36" pin="GNDIO" pad="20"/>
<connect gate="37" pin="GNDIO" pad="32"/>
<connect gate="38" pin="GNDIO" pad="48"/>
<connect gate="39" pin="GNDIO" pad="59"/>
<connect gate="4" pin="VCC" pad="43"/>
<connect gate="40" pin="GNDIO" pad="72"/>
<connect gate="41" pin="GNDIO" pad="91"/>
<connect gate="42" pin="GNDIO" pad="124"/>
<connect gate="43" pin="GNDIO" pad="130"/>
<connect gate="44" pin="GNDIO" pad="152"/>
<connect gate="45" pin="GNDIO" pad="171"/>
<connect gate="46" pin="GNDIO" pad="188"/>
<connect gate="47" pin="GNDIO" pad="201"/>
<connect gate="5" pin="VCC" pad="76"/>
<connect gate="6" pin="VCC" pad="77"/>
<connect gate="7" pin="VCC" pad="106"/>
<connect gate="8" pin="VCC" pad="109"/>
<connect gate="9" pin="VCC" pad="117"/>
<connect gate="_" pin="/CE" pad="154"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="105"/>
<connect gate="_" pin="/STATUS" pad="52"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="156"/>
<connect gate="_" pin="DCLK" pad="155"/>
<connect gate="_" pin="GCLK0" pad="183"/>
<connect gate="_" pin="GCLK1" pad="79"/>
<connect gate="_" pin="IN0" pad="78"/>
<connect gate="_" pin="IN1" pad="80"/>
<connect gate="_" pin="IN2" pad="182"/>
<connect gate="_" pin="IN3" pad="184"/>
<connect gate="_" pin="MSEL0" pad="108"/>
<connect gate="_" pin="MSEL1" pad="107"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="153"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="50"/>
<connect gate="_" pin="TRST" pad="51"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K20RC208-3N"/>
<attribute name="OC_FARNELL" value="1549383"/>
<attribute name="OC_NEWARK" value="51R8880"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K10-P208" prefix="IC">
<description>&lt;b&gt;EPF10K10&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="K10-CTRL"/>
<gate name="-A" symbol="A16"/>
<gate name="-B" symbol="B16"/>
<gate name="-C" symbol="C16"/>
<gate name="-1" symbol="52-K10"/>
<gate name="-2" symbol="102-K10"/>
<gate name="-3" symbol="151-K10"/>
<gate name="-4" symbol="201-K10"/>
<gate name="-5" symbol="244-K10"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
<gate name="7" symbol="VCCINT"/>
<gate name="8" symbol="VCCINT"/>
<gate name="9" symbol="VCCINT"/>
<gate name="10" symbol="VCCINT"/>
<gate name="11" symbol="VCCINT"/>
<gate name="12" symbol="VCCINT"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="19" symbol="VCCIO"/>
<gate name="20" symbol="VCCIO"/>
<gate name="21" symbol="VCCIO"/>
<gate name="22" symbol="VCCIO"/>
<gate name="23" symbol="VCCIO"/>
<gate name="24" symbol="VCCIO"/>
<gate name="25" symbol="VCCIO"/>
<gate name="26" symbol="VCCIO"/>
<gate name="27" symbol="GNDINT"/>
<gate name="28" symbol="GNDINT"/>
<gate name="29" symbol="GNDINT"/>
<gate name="30" symbol="GNDINT"/>
<gate name="31" symbol="GNDINT"/>
<gate name="32" symbol="GNDINT"/>
<gate name="33" symbol="GNDINT"/>
<gate name="34" symbol="GNDINT"/>
<gate name="35" symbol="GNDINT"/>
<gate name="36" symbol="GNDIO"/>
<gate name="37" symbol="GNDIO"/>
<gate name="38" symbol="GNDIO"/>
<gate name="39" symbol="GNDIO"/>
<gate name="40" symbol="GNDIO"/>
<gate name="41" symbol="GNDIO"/>
<gate name="42" symbol="GNDIO"/>
<gate name="43" symbol="GNDIO"/>
<gate name="44" symbol="GNDIO"/>
<gate name="45" symbol="GNDIO"/>
<gate name="46" symbol="GNDIO"/>
<gate name="47" symbol="GNDIO"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="-1" pin="IO11" pad="103"/>
<connect gate="-1" pin="IO12" pad="104"/>
<connect gate="-1" pin="IO13" pad="157"/>
<connect gate="-1" pin="IO14" pad="158"/>
<connect gate="-1" pin="IO21" pad="102"/>
<connect gate="-1" pin="IO22" pad="159"/>
<connect gate="-1" pin="IO23" pad="160"/>
<connect gate="-1" pin="IO31" pad="100"/>
<connect gate="-1" pin="IO32" pad="101"/>
<connect gate="-1" pin="IO33" pad="161"/>
<connect gate="-1" pin="IO34" pad="162"/>
<connect gate="-1" pin="IO41" pad="99"/>
<connect gate="-1" pin="IO42" pad="163"/>
<connect gate="-1" pin="IO43" pad="164"/>
<connect gate="-1" pin="IO51" pad="96"/>
<connect gate="-1" pin="IO52" pad="97"/>
<connect gate="-2" pin="IO101" pad="87"/>
<connect gate="-2" pin="IO102" pad="88"/>
<connect gate="-2" pin="IO53" pad="166"/>
<connect gate="-2" pin="IO61" pad="95"/>
<connect gate="-2" pin="IO62" pad="167"/>
<connect gate="-2" pin="IO63" pad="168"/>
<connect gate="-2" pin="IO71" pad="93"/>
<connect gate="-2" pin="IO72" pad="94"/>
<connect gate="-2" pin="IO73" pad="169"/>
<connect gate="-2" pin="IO81" pad="90"/>
<connect gate="-2" pin="IO82" pad="92"/>
<connect gate="-2" pin="IO83" pad="170"/>
<connect gate="-2" pin="IO84" pad="172"/>
<connect gate="-2" pin="IO91" pad="89"/>
<connect gate="-2" pin="IO92" pad="173"/>
<connect gate="-2" pin="IO93" pad="174"/>
<connect gate="-3" pin="IO103" pad="175"/>
<connect gate="-3" pin="IO111" pad="85"/>
<connect gate="-3" pin="IO112" pad="86"/>
<connect gate="-3" pin="IO113" pad="176"/>
<connect gate="-3" pin="IO114" pad="177"/>
<connect gate="-3" pin="IO121" pad="83"/>
<connect gate="-3" pin="IO122" pad="179"/>
<connect gate="-3" pin="IO123" pad="180"/>
<connect gate="-3" pin="IO131" pad="74"/>
<connect gate="-3" pin="IO132" pad="75"/>
<connect gate="-3" pin="IO133" pad="186"/>
<connect gate="-3" pin="IO134" pad="187"/>
<connect gate="-3" pin="IO141" pad="71"/>
<connect gate="-3" pin="IO142" pad="73"/>
<connect gate="-3" pin="IO143" pad="189"/>
<connect gate="-3" pin="IO151" pad="70"/>
<connect gate="-4" pin="IO152" pad="190"/>
<connect gate="-4" pin="IO153" pad="191"/>
<connect gate="-4" pin="IO161" pad="68"/>
<connect gate="-4" pin="IO162" pad="69"/>
<connect gate="-4" pin="IO163" pad="192"/>
<connect gate="-4" pin="IO171" pad="67"/>
<connect gate="-4" pin="IO172" pad="193"/>
<connect gate="-4" pin="IO173" pad="195"/>
<connect gate="-4" pin="IO181" pad="64"/>
<connect gate="-4" pin="IO182" pad="65"/>
<connect gate="-4" pin="IO183" pad="196"/>
<connect gate="-4" pin="IO184" pad="197"/>
<connect gate="-4" pin="IO191" pad="62"/>
<connect gate="-4" pin="IO192" pad="63"/>
<connect gate="-4" pin="IO193" pad="198"/>
<connect gate="-4" pin="IO201" pad="61"/>
<connect gate="-5" pin="IO202" pad="199"/>
<connect gate="-5" pin="IO203" pad="200"/>
<connect gate="-5" pin="IO211" pad="58"/>
<connect gate="-5" pin="IO212" pad="60"/>
<connect gate="-5" pin="IO213" pad="202"/>
<connect gate="-5" pin="IO214" pad="203"/>
<connect gate="-5" pin="IO221" pad="56"/>
<connect gate="-5" pin="IO222" pad="57"/>
<connect gate="-5" pin="IO223" pad="204"/>
<connect gate="-5" pin="IO231" pad="55"/>
<connect gate="-5" pin="IO232" pad="205"/>
<connect gate="-5" pin="IO233" pad="206"/>
<connect gate="-5" pin="IO241" pad="53"/>
<connect gate="-5" pin="IO242" pad="54"/>
<connect gate="-5" pin="IO243" pad="207"/>
<connect gate="-5" pin="IO244" pad="208"/>
<connect gate="-A" pin="IOA1" pad="10"/>
<connect gate="-A" pin="IOA10" pad="142"/>
<connect gate="-A" pin="IOA11" pad="143"/>
<connect gate="-A" pin="IOA12" pad="144"/>
<connect gate="-A" pin="IOA13" pad="147"/>
<connect gate="-A" pin="IOA14" pad="148"/>
<connect gate="-A" pin="IOA15" pad="149"/>
<connect gate="-A" pin="IOA16" pad="150"/>
<connect gate="-A" pin="IOA2" pad="11"/>
<connect gate="-A" pin="IOA3" pad="12"/>
<connect gate="-A" pin="IOA4" pad="13"/>
<connect gate="-A" pin="IOA5" pad="16"/>
<connect gate="-A" pin="IOA6" pad="17"/>
<connect gate="-A" pin="IOA7" pad="18"/>
<connect gate="-A" pin="IOA8" pad="19"/>
<connect gate="-A" pin="IOA9" pad="141"/>
<connect gate="-B" pin="IOB1" pad="24"/>
<connect gate="-B" pin="IOB10" pad="128"/>
<connect gate="-B" pin="IOB11" pad="131"/>
<connect gate="-B" pin="IOB12" pad="132"/>
<connect gate="-B" pin="IOB13" pad="133"/>
<connect gate="-B" pin="IOB14" pad="134"/>
<connect gate="-B" pin="IOB15" pad="135"/>
<connect gate="-B" pin="IOB16" pad="136"/>
<connect gate="-B" pin="IOB2" pad="25"/>
<connect gate="-B" pin="IOB3" pad="26"/>
<connect gate="-B" pin="IOB4" pad="27"/>
<connect gate="-B" pin="IOB5" pad="28"/>
<connect gate="-B" pin="IOB6" pad="29"/>
<connect gate="-B" pin="IOB7" pad="30"/>
<connect gate="-B" pin="IOB8" pad="31"/>
<connect gate="-B" pin="IOB9" pad="127"/>
<connect gate="-C" pin="IOC1" pad="38"/>
<connect gate="-C" pin="IOC10" pad="112"/>
<connect gate="-C" pin="IOC11" pad="115"/>
<connect gate="-C" pin="IOC12" pad="116"/>
<connect gate="-C" pin="IOC13" pad="119"/>
<connect gate="-C" pin="IOC14" pad="120"/>
<connect gate="-C" pin="IOC15" pad="121"/>
<connect gate="-C" pin="IOC16" pad="122"/>
<connect gate="-C" pin="IOC2" pad="39"/>
<connect gate="-C" pin="IOC3" pad="40"/>
<connect gate="-C" pin="IOC4" pad="41"/>
<connect gate="-C" pin="IOC5" pad="44"/>
<connect gate="-C" pin="IOC6" pad="45"/>
<connect gate="-C" pin="IOC7" pad="46"/>
<connect gate="-C" pin="IOC8" pad="47"/>
<connect gate="-C" pin="IOC9" pad="111"/>
<connect gate="1" pin="VCC" pad="6"/>
<connect gate="10" pin="VCC" pad="137"/>
<connect gate="11" pin="VCC" pad="145"/>
<connect gate="12" pin="VCC" pad="181"/>
<connect gate="13" pin="VCCIO" pad="5"/>
<connect gate="14" pin="VCCIO" pad="22"/>
<connect gate="15" pin="VCCIO" pad="34"/>
<connect gate="16" pin="VCCIO" pad="42"/>
<connect gate="17" pin="VCCIO" pad="66"/>
<connect gate="18" pin="VCCIO" pad="84"/>
<connect gate="19" pin="VCCIO" pad="98"/>
<connect gate="2" pin="VCC" pad="23"/>
<connect gate="20" pin="VCCIO" pad="110"/>
<connect gate="21" pin="VCCIO" pad="118"/>
<connect gate="22" pin="VCCIO" pad="138"/>
<connect gate="23" pin="VCCIO" pad="146"/>
<connect gate="24" pin="VCCIO" pad="165"/>
<connect gate="25" pin="VCCIO" pad="178"/>
<connect gate="26" pin="VCCIO" pad="194"/>
<connect gate="27" pin="GND" pad="21"/>
<connect gate="28" pin="GND" pad="33"/>
<connect gate="29" pin="GND" pad="49"/>
<connect gate="3" pin="VCC" pad="35"/>
<connect gate="30" pin="GND" pad="81"/>
<connect gate="31" pin="GND" pad="82"/>
<connect gate="32" pin="GND" pad="123"/>
<connect gate="33" pin="GND" pad="129"/>
<connect gate="34" pin="GND" pad="151"/>
<connect gate="35" pin="GND" pad="185"/>
<connect gate="36" pin="GNDIO" pad="20"/>
<connect gate="37" pin="GNDIO" pad="32"/>
<connect gate="38" pin="GNDIO" pad="48"/>
<connect gate="39" pin="GNDIO" pad="59"/>
<connect gate="4" pin="VCC" pad="43"/>
<connect gate="40" pin="GNDIO" pad="72"/>
<connect gate="41" pin="GNDIO" pad="91"/>
<connect gate="42" pin="GNDIO" pad="124"/>
<connect gate="43" pin="GNDIO" pad="130"/>
<connect gate="44" pin="GNDIO" pad="152"/>
<connect gate="45" pin="GNDIO" pad="171"/>
<connect gate="46" pin="GNDIO" pad="188"/>
<connect gate="47" pin="GNDIO" pad="201"/>
<connect gate="5" pin="VCC" pad="76"/>
<connect gate="6" pin="VCC" pad="77"/>
<connect gate="7" pin="VCC" pad="106"/>
<connect gate="8" pin="VCC" pad="109"/>
<connect gate="9" pin="VCC" pad="117"/>
<connect gate="NC1" pin="NC" pad="7"/>
<connect gate="NC10" pin="NC" pad="125"/>
<connect gate="NC11" pin="NC" pad="126"/>
<connect gate="NC12" pin="NC" pad="139"/>
<connect gate="NC13" pin="NC" pad="140"/>
<connect gate="NC2" pin="NC" pad="8"/>
<connect gate="NC3" pin="NC" pad="9"/>
<connect gate="NC4" pin="NC" pad="14"/>
<connect gate="NC5" pin="NC" pad="15"/>
<connect gate="NC6" pin="NC" pad="36"/>
<connect gate="NC7" pin="NC" pad="37"/>
<connect gate="NC8" pin="NC" pad="113"/>
<connect gate="NC9" pin="NC" pad="114"/>
<connect gate="_" pin="/CE" pad="154"/>
<connect gate="_" pin="/CEO" pad="3"/>
<connect gate="_" pin="/CONFIG" pad="105"/>
<connect gate="_" pin="/STATUS" pad="52"/>
<connect gate="_" pin="CONF_DONE" pad="2"/>
<connect gate="_" pin="DATA0" pad="156"/>
<connect gate="_" pin="DCLK" pad="155"/>
<connect gate="_" pin="GCLK0" pad="79"/>
<connect gate="_" pin="GCLK1" pad="183"/>
<connect gate="_" pin="IN0" pad="78"/>
<connect gate="_" pin="IN1" pad="80"/>
<connect gate="_" pin="IN2" pad="182"/>
<connect gate="_" pin="IN3" pad="184"/>
<connect gate="_" pin="MSEL0" pad="108"/>
<connect gate="_" pin="MSEL1" pad="107"/>
<connect gate="_" pin="TCK" pad="1"/>
<connect gate="_" pin="TDI" pad="153"/>
<connect gate="_" pin="TDO" pad="4"/>
<connect gate="_" pin="TMS" pad="50"/>
<connect gate="_" pin="TRST" pad="51"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K10AQC208-3N"/>
<attribute name="OC_FARNELL" value="1549381"/>
<attribute name="OC_NEWARK" value="51R8749"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF10K30-BGA356" prefix="IC">
<description>&lt;b&gt;EPF10K30&lt;/b&gt;&lt;p&gt;
FLEX 10K family</description>
<gates>
<gate name="_" symbol="100R240C"/>
<gate name="-A" symbol="A16"/>
<gate name="-B" symbol="B16"/>
<gate name="-C" symbol="C16"/>
<gate name="-D" symbol="D16"/>
<gate name="-E" symbol="E16"/>
<gate name="-1" symbol="IO44"/>
<gate name="-2" symbol="IO84"/>
<gate name="-3" symbol="IO124"/>
<gate name="-4" symbol="IO164"/>
<gate name="-5" symbol="IO204"/>
<gate name="-6" symbol="IO244"/>
<gate name="-7" symbol="IO284"/>
<gate name="-8" symbol="IO324"/>
<gate name="-9" symbol="IO364"/>
<gate name="-F" symbol="F16"/>
<gate name="G1" symbol="GNDINT"/>
<gate name="G2" symbol="GNDINT"/>
<gate name="G3" symbol="GNDINT"/>
<gate name="G4" symbol="GNDINT"/>
<gate name="G5" symbol="GNDINT"/>
<gate name="G6" symbol="GNDINT"/>
<gate name="G7" symbol="GNDINT"/>
<gate name="G8" symbol="GNDINT"/>
<gate name="G9" symbol="GNDINT"/>
<gate name="G10" symbol="GNDINT"/>
<gate name="G11" symbol="GNDINT"/>
<gate name="G12" symbol="GNDINT"/>
<gate name="G13" symbol="GNDINT"/>
<gate name="G14" symbol="GNDINT"/>
<gate name="G15" symbol="GNDINT"/>
<gate name="G16" symbol="GNDINT"/>
<gate name="G17" symbol="GNDINT"/>
<gate name="G18" symbol="GNDINT"/>
<gate name="G19" symbol="GNDINT"/>
<gate name="G20" symbol="GNDINT"/>
<gate name="G21" symbol="GNDINT"/>
<gate name="G22" symbol="GNDINT"/>
<gate name="G23" symbol="GNDINT"/>
<gate name="G24" symbol="GNDINT"/>
<gate name="G25" symbol="GNDINT"/>
<gate name="G26" symbol="GNDINT"/>
<gate name="G27" symbol="GNDINT"/>
<gate name="G28" symbol="GNDINT"/>
<gate name="G29" symbol="GNDINT"/>
<gate name="G30" symbol="GNDINT"/>
<gate name="G31" symbol="GNDINT"/>
<gate name="G32" symbol="GNDINT"/>
<gate name="G33" symbol="GNDINT"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
<gate name="NC17" symbol="NC"/>
<gate name="NC18" symbol="NC"/>
<gate name="NC19" symbol="NC"/>
<gate name="NC20" symbol="NC"/>
<gate name="NC21" symbol="NC"/>
<gate name="NC22" symbol="NC"/>
<gate name="NC23" symbol="NC"/>
<gate name="NC24" symbol="NC"/>
<gate name="NC25" symbol="NC"/>
<gate name="NC26" symbol="NC"/>
<gate name="NC27" symbol="NC"/>
<gate name="NC28" symbol="NC"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="V5" symbol="VCCINT"/>
<gate name="V6" symbol="VCCINT"/>
<gate name="V7" symbol="VCCINT"/>
<gate name="V8" symbol="VCCINT"/>
<gate name="V9" symbol="VCCINT"/>
<gate name="V10" symbol="VCCINT"/>
<gate name="V11" symbol="VCCINT"/>
<gate name="V12" symbol="VCCINT"/>
<gate name="V13" symbol="VCCINT"/>
<gate name="V14" symbol="VCCINT"/>
<gate name="V15" symbol="VCCINT"/>
<gate name="V16" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="VO11" symbol="VCCIO"/>
<gate name="VO12" symbol="VCCIO"/>
<gate name="VO13" symbol="VCCIO"/>
<gate name="VO14" symbol="VCCIO"/>
<gate name="VO15" symbol="VCCIO"/>
<gate name="VO16" symbol="VCCIO"/>
<gate name="VO17" symbol="VCCIO"/>
<gate name="VO18" symbol="VCCIO"/>
<gate name="VO19" symbol="VCCIO"/>
</gates>
<devices>
<device name="" package="BGA356">
<connects>
<connect gate="-1" pin="IO11" pad="C4"/>
<connect gate="-1" pin="IO12" pad="AD4"/>
<connect gate="-1" pin="IO13" pad="Y4"/>
<connect gate="-1" pin="IO14" pad="C3"/>
<connect gate="-1" pin="IO21" pad="C5"/>
<connect gate="-1" pin="IO22" pad="G2"/>
<connect gate="-1" pin="IO23" pad="AD5"/>
<connect gate="-1" pin="IO24" pad="AE3"/>
<connect gate="-1" pin="IO31" pad="B3"/>
<connect gate="-1" pin="IO32" pad="AF2"/>
<connect gate="-1" pin="IO33" pad="Y3"/>
<connect gate="-1" pin="IO34" pad="B2"/>
<connect gate="-1" pin="IO41" pad="C6"/>
<connect gate="-1" pin="IO42" pad="AE4"/>
<connect gate="-1" pin="IO43" pad="AD6"/>
<connect gate="-1" pin="IO44" pad="G4"/>
<connect gate="-2" pin="IO51" pad="A3"/>
<connect gate="-2" pin="IO52" pad="B5"/>
<connect gate="-2" pin="IO53" pad="AE5"/>
<connect gate="-2" pin="IO54" pad="AA2"/>
<connect gate="-2" pin="IO61" pad="F5"/>
<connect gate="-2" pin="IO62" pad="AD7"/>
<connect gate="-2" pin="IO63" pad="AD8"/>
<connect gate="-2" pin="IO64" pad="C7"/>
<connect gate="-2" pin="IO71" pad="A4"/>
<connect gate="-2" pin="IO72" pad="B6"/>
<connect gate="-2" pin="IO73" pad="AF4"/>
<connect gate="-2" pin="IO74" pad="AA3"/>
<connect gate="-2" pin="IO81" pad="C8"/>
<connect gate="-2" pin="IO82" pad="AE6"/>
<connect gate="-2" pin="IO83" pad="AD9"/>
<connect gate="-2" pin="IO84" pad="G3"/>
<connect gate="-3" pin="IO101" pad="B7"/>
<connect gate="-3" pin="IO102" pad="AD10"/>
<connect gate="-3" pin="IO103" pad="AF5"/>
<connect gate="-3" pin="IO104" pad="F2"/>
<connect gate="-3" pin="IO111" pad="B9"/>
<connect gate="-3" pin="IO112" pad="AB2"/>
<connect gate="-3" pin="IO113" pad="AE9"/>
<connect gate="-3" pin="IO114" pad="C10"/>
<connect gate="-3" pin="IO121" pad="A6"/>
<connect gate="-3" pin="IO122" pad="F3"/>
<connect gate="-3" pin="IO123" pad="AE10"/>
<connect gate="-3" pin="IO124" pad="AF6"/>
<connect gate="-3" pin="IO91" pad="B8"/>
<connect gate="-3" pin="IO92" pad="A5"/>
<connect gate="-3" pin="IO93" pad="AE8"/>
<connect gate="-3" pin="IO94" pad="AA4"/>
<connect gate="-4" pin="IO131" pad="B10"/>
<connect gate="-4" pin="IO132" pad="C11"/>
<connect gate="-4" pin="IO133" pad="AD11"/>
<connect gate="-4" pin="IO134" pad="AB3"/>
<connect gate="-4" pin="IO141" pad="A8"/>
<connect gate="-4" pin="IO142" pad="AF8"/>
<connect gate="-4" pin="IO143" pad="AF9"/>
<connect gate="-4" pin="IO144" pad="E5"/>
<connect gate="-4" pin="IO151" pad="B11"/>
<connect gate="-4" pin="IO152" pad="AB4"/>
<connect gate="-4" pin="IO153" pad="AE11"/>
<connect gate="-4" pin="IO154" pad="A9"/>
<connect gate="-4" pin="IO161" pad="C12"/>
<connect gate="-4" pin="IO162" pad="AD12"/>
<connect gate="-4" pin="IO163" pad="E4"/>
<connect gate="-4" pin="IO164" pad="AF10"/>
<connect gate="-5" pin="IO171" pad="B12"/>
<connect gate="-5" pin="IO172" pad="AC1"/>
<connect gate="-5" pin="IO173" pad="AE12"/>
<connect gate="-5" pin="IO174" pad="A11"/>
<connect gate="-5" pin="IO181" pad="A12"/>
<connect gate="-5" pin="IO182" pad="AF12"/>
<connect gate="-5" pin="IO183" pad="AD13"/>
<connect gate="-5" pin="IO184" pad="E3"/>
<connect gate="-5" pin="IO191" pad="B15"/>
<connect gate="-5" pin="IO192" pad="A15"/>
<connect gate="-5" pin="IO193" pad="AE14"/>
<connect gate="-5" pin="IO194" pad="AB25"/>
<connect gate="-5" pin="IO201" pad="A16"/>
<connect gate="-5" pin="IO202" pad="AF15"/>
<connect gate="-5" pin="IO203" pad="AE15"/>
<connect gate="-5" pin="IO204" pad="E24"/>
<connect gate="-6" pin="IO211" pad="B16"/>
<connect gate="-6" pin="IO212" pad="A17"/>
<connect gate="-6" pin="IO213" pad="AD15"/>
<connect gate="-6" pin="IO214" pad="AB24"/>
<connect gate="-6" pin="IO221" pad="A18"/>
<connect gate="-6" pin="IO222" pad="AF17"/>
<connect gate="-6" pin="IO223" pad="AE16"/>
<connect gate="-6" pin="IO224" pad="E25"/>
<connect gate="-6" pin="IO231" pad="C16"/>
<connect gate="-6" pin="IO232" pad="AB23"/>
<connect gate="-6" pin="IO233" pad="AF18"/>
<connect gate="-6" pin="IO234" pad="B17"/>
<connect gate="-6" pin="IO241" pad="A19"/>
<connect gate="-6" pin="IO242" pad="AD16"/>
<connect gate="-6" pin="IO243" pad="AE17"/>
<connect gate="-6" pin="IO244" pad="E26"/>
<connect gate="-7" pin="IO251" pad="C17"/>
<connect gate="-7" pin="IO252" pad="B18"/>
<connect gate="-7" pin="IO253" pad="AF20"/>
<connect gate="-7" pin="IO254" pad="AB26"/>
<connect gate="-7" pin="IO261" pad="A21"/>
<connect gate="-7" pin="IO262" pad="F25"/>
<connect gate="-7" pin="IO263" pad="AD17"/>
<connect gate="-7" pin="IO264" pad="AE18"/>
<connect gate="-7" pin="IO271" pad="A22"/>
<connect gate="-7" pin="IO272" pad="AA25"/>
<connect gate="-7" pin="IO273" pad="AF21"/>
<connect gate="-7" pin="IO274" pad="B19"/>
<connect gate="-7" pin="IO281" pad="C18"/>
<connect gate="-7" pin="IO282" pad="AE19"/>
<connect gate="-7" pin="IO283" pad="F24"/>
<connect gate="-7" pin="IO284" pad="AF22"/>
<connect gate="-8" pin="IO291" pad="A24"/>
<connect gate="-8" pin="IO292" pad="B20"/>
<connect gate="-8" pin="IO293" pad="AF23"/>
<connect gate="-8" pin="IO294" pad="AA26"/>
<connect gate="-8" pin="IO301" pad="F23"/>
<connect gate="-8" pin="IO302" pad="AE20"/>
<connect gate="-8" pin="IO303" pad="AE21"/>
<connect gate="-8" pin="IO304" pad="C19"/>
<connect gate="-8" pin="IO311" pad="A25"/>
<connect gate="-8" pin="IO312" pad="B21"/>
<connect gate="-8" pin="IO313" pad="AD19"/>
<connect gate="-8" pin="IO314" pad="Y26"/>
<connect gate="-8" pin="IO321" pad="C20"/>
<connect gate="-8" pin="IO322" pad="AF24"/>
<connect gate="-8" pin="IO323" pad="AE22"/>
<connect gate="-8" pin="IO324" pad="F26"/>
<connect gate="-9" pin="IO331" pad="C21"/>
<connect gate="-9" pin="IO332" pad="AE23"/>
<connect gate="-9" pin="IO333" pad="Y24"/>
<connect gate="-9" pin="IO334" pad="B23"/>
<connect gate="-9" pin="IO341" pad="B24"/>
<connect gate="-9" pin="IO342" pad="AD21"/>
<connect gate="-9" pin="IO343" pad="AE24"/>
<connect gate="-9" pin="IO344" pad="G25"/>
<connect gate="-9" pin="IO351" pad="C22"/>
<connect gate="-9" pin="IO352" pad="AD23"/>
<connect gate="-9" pin="IO353" pad="C23"/>
<connect gate="-9" pin="IO354" pad="Y25"/>
<connect gate="-9" pin="IO361" pad="C24"/>
<connect gate="-9" pin="IO362" pad="G24"/>
<connect gate="-9" pin="IO363" pad="AD24"/>
<connect gate="-9" pin="IO364" pad="AD22"/>
<connect gate="-A" pin="IOA1" pad="AB22"/>
<connect gate="-A" pin="IOA10" pad="Y5"/>
<connect gate="-A" pin="IOA11" pad="AA5"/>
<connect gate="-A" pin="IOA12" pad="AB5"/>
<connect gate="-A" pin="IOA13" pad="AC4"/>
<connect gate="-A" pin="IOA14" pad="W25"/>
<connect gate="-A" pin="IOA15" pad="AD1"/>
<connect gate="-A" pin="IOA16" pad="W4"/>
<connect gate="-A" pin="IOA2" pad="AA22"/>
<connect gate="-A" pin="IOA3" pad="AA23"/>
<connect gate="-A" pin="IOA4" pad="Y22"/>
<connect gate="-A" pin="IOA5" pad="AA24"/>
<connect gate="-A" pin="IOA6" pad="W23"/>
<connect gate="-A" pin="IOA7" pad="W24"/>
<connect gate="-A" pin="IOA8" pad="V5"/>
<connect gate="-A" pin="IOA9" pad="W5"/>
<connect gate="-B" pin="IOB1" pad="V22"/>
<connect gate="-B" pin="IOB10" pad="T5"/>
<connect gate="-B" pin="IOB11" pad="U1"/>
<connect gate="-B" pin="IOB12" pad="U2"/>
<connect gate="-B" pin="IOB13" pad="U3"/>
<connect gate="-B" pin="IOB14" pad="U4"/>
<connect gate="-B" pin="IOB15" pad="T22"/>
<connect gate="-B" pin="IOB16" pad="T3"/>
<connect gate="-B" pin="IOB2" pad="V23"/>
<connect gate="-B" pin="IOB3" pad="W26"/>
<connect gate="-B" pin="IOB4" pad="V24"/>
<connect gate="-B" pin="IOB5" pad="V25"/>
<connect gate="-B" pin="IOB6" pad="U23"/>
<connect gate="-B" pin="IOB7" pad="U24"/>
<connect gate="-B" pin="IOB8" pad="T2"/>
<connect gate="-B" pin="IOB9" pad="T4"/>
<connect gate="-C" pin="IOC1" pad="U22"/>
<connect gate="-C" pin="IOC10" pad="P1"/>
<connect gate="-C" pin="IOC11" pad="R2"/>
<connect gate="-C" pin="IOC12" pad="R4"/>
<connect gate="-C" pin="IOC13" pad="R5"/>
<connect gate="-C" pin="IOC14" pad="R3"/>
<connect gate="-C" pin="IOC15" pad="P5"/>
<connect gate="-C" pin="IOC16" pad="P25"/>
<connect gate="-C" pin="IOC2" pad="R22"/>
<connect gate="-C" pin="IOC3" pad="R23"/>
<connect gate="-C" pin="IOC4" pad="T24"/>
<connect gate="-C" pin="IOC5" pad="R25"/>
<connect gate="-C" pin="IOC6" pad="P22"/>
<connect gate="-C" pin="IOC7" pad="P23"/>
<connect gate="-C" pin="IOC8" pad="P4"/>
<connect gate="-C" pin="IOC9" pad="P3"/>
<connect gate="-D" pin="IOD1" pad="P26"/>
<connect gate="-D" pin="IOD10" pad="M2"/>
<connect gate="-D" pin="IOD11" pad="N2"/>
<connect gate="-D" pin="IOD12" pad="N4"/>
<connect gate="-D" pin="IOD13" pad="N5"/>
<connect gate="-D" pin="IOD14" pad="N3"/>
<connect gate="-D" pin="IOD15" pad="M5"/>
<connect gate="-D" pin="IOD16" pad="M22"/>
<connect gate="-D" pin="IOD2" pad="N25"/>
<connect gate="-D" pin="IOD3" pad="N22"/>
<connect gate="-D" pin="IOD4" pad="N23"/>
<connect gate="-D" pin="IOD5" pad="N24"/>
<connect gate="-D" pin="IOD6" pad="M25"/>
<connect gate="-D" pin="IOD7" pad="M24"/>
<connect gate="-D" pin="IOD8" pad="M4"/>
<connect gate="-D" pin="IOD9" pad="M3"/>
<connect gate="-E" pin="IOE1" pad="L26"/>
<connect gate="-E" pin="IOE10" pad="L4"/>
<connect gate="-E" pin="IOE11" pad="L5"/>
<connect gate="-E" pin="IOE12" pad="K2"/>
<connect gate="-E" pin="IOE13" pad="L2"/>
<connect gate="-E" pin="IOE14" pad="L1"/>
<connect gate="-E" pin="IOE15" pad="K3"/>
<connect gate="-E" pin="IOE16" pad="K23"/>
<connect gate="-E" pin="IOE2" pad="L24"/>
<connect gate="-E" pin="IOE3" pad="L22"/>
<connect gate="-E" pin="IOE4" pad="L23"/>
<connect gate="-E" pin="IOE5" pad="L25"/>
<connect gate="-E" pin="IOE6" pad="K26"/>
<connect gate="-E" pin="IOE7" pad="K22"/>
<connect gate="-E" pin="IOE8" pad="K4"/>
<connect gate="-E" pin="IOE9" pad="L3"/>
<connect gate="-F" pin="IOF1" pad="J22"/>
<connect gate="-F" pin="IOF10" pad="H2"/>
<connect gate="-F" pin="IOF11" pad="J5"/>
<connect gate="-F" pin="IOF12" pad="J4"/>
<connect gate="-F" pin="IOF13" pad="J3"/>
<connect gate="-F" pin="IOF14" pad="J2"/>
<connect gate="-F" pin="IOF15" pad="H4"/>
<connect gate="-F" pin="IOF16" pad="E22"/>
<connect gate="-F" pin="IOF2" pad="K24"/>
<connect gate="-F" pin="IOF3" pad="J23"/>
<connect gate="-F" pin="IOF4" pad="J24"/>
<connect gate="-F" pin="IOF5" pad="G22"/>
<connect gate="-F" pin="IOF6" pad="F22"/>
<connect gate="-F" pin="IOF7" pad="E23"/>
<connect gate="-F" pin="IOF8" pad="H5"/>
<connect gate="-F" pin="IOF9" pad="H3"/>
<connect gate="G1" pin="GND" pad="AD2"/>
<connect gate="G10" pin="GND" pad="AF19"/>
<connect gate="G11" pin="GND" pad="B25"/>
<connect gate="G12" pin="GND" pad="B22"/>
<connect gate="G13" pin="GND" pad="B13"/>
<connect gate="G14" pin="GND" pad="B1"/>
<connect gate="G15" pin="GND" pad="A20"/>
<connect gate="G16" pin="GND" pad="A10"/>
<connect gate="G17" pin="GND" pad="A2"/>
<connect gate="G18" pin="GND" pad="AF25"/>
<connect gate="G19" pin="GND" pad="B26"/>
<connect gate="G2" pin="GND" pad="AD14"/>
<connect gate="G20" pin="GND" pad="C2"/>
<connect gate="G21" pin="GND" pad="C9"/>
<connect gate="G22" pin="GND" pad="C13"/>
<connect gate="G23" pin="GND" pad="C25"/>
<connect gate="G24" pin="GND" pad="H23"/>
<connect gate="G25" pin="GND" pad="J26"/>
<connect gate="G26" pin="GND" pad="K1"/>
<connect gate="G27" pin="GND" pad="M1"/>
<connect gate="G28" pin="GND" pad="N26"/>
<connect gate="G29" pin="GND" pad="R1"/>
<connect gate="G3" pin="GND" pad="AD20"/>
<connect gate="G30" pin="GND" pad="R26"/>
<connect gate="G31" pin="GND" pad="T1"/>
<connect gate="G32" pin="GND" pad="U26"/>
<connect gate="G33" pin="GND" pad="W1"/>
<connect gate="G4" pin="GND" pad="AE1"/>
<connect gate="G5" pin="GND" pad="AE2"/>
<connect gate="G6" pin="GND" pad="AE7"/>
<connect gate="G7" pin="GND" pad="AE25"/>
<connect gate="G8" pin="GND" pad="AE26"/>
<connect gate="G9" pin="GND" pad="AF11"/>
<connect gate="NC1" pin="NC" pad="AC26"/>
<connect gate="NC10" pin="NC" pad="G26"/>
<connect gate="NC11" pin="NC" pad="H1"/>
<connect gate="NC12" pin="NC" pad="H25"/>
<connect gate="NC13" pin="NC" pad="H26"/>
<connect gate="NC14" pin="NC" pad="J25"/>
<connect gate="NC15" pin="NC" pad="K25"/>
<connect gate="NC16" pin="NC" pad="P24"/>
<connect gate="NC17" pin="NC" pad="R24"/>
<connect gate="NC18" pin="NC" pad="T23"/>
<connect gate="NC19" pin="NC" pad="U25"/>
<connect gate="NC2" pin="NC" pad="C1"/>
<connect gate="NC20" pin="NC" pad="V1"/>
<connect gate="NC21" pin="NC" pad="V3"/>
<connect gate="NC22" pin="NC" pad="V4"/>
<connect gate="NC23" pin="NC" pad="V26"/>
<connect gate="NC24" pin="NC" pad="W2"/>
<connect gate="NC25" pin="NC" pad="W3"/>
<connect gate="NC26" pin="NC" pad="Y1"/>
<connect gate="NC27" pin="NC" pad="Y2"/>
<connect gate="NC28" pin="NC" pad="Y23"/>
<connect gate="NC3" pin="NC" pad="D1"/>
<connect gate="NC4" pin="NC" pad="D26"/>
<connect gate="NC5" pin="NC" pad="E1"/>
<connect gate="NC6" pin="NC" pad="E2"/>
<connect gate="NC7" pin="NC" pad="G1"/>
<connect gate="NC8" pin="NC" pad="G5"/>
<connect gate="NC9" pin="NC" pad="G23"/>
<connect gate="V1" pin="VCC" pad="AA1"/>
<connect gate="V10" pin="VCC" pad="F1"/>
<connect gate="V11" pin="VCC" pad="H22"/>
<connect gate="V12" pin="VCC" pad="J1"/>
<connect gate="V13" pin="VCC" pad="M26"/>
<connect gate="V14" pin="VCC" pad="N1"/>
<connect gate="V15" pin="VCC" pad="T26"/>
<connect gate="V16" pin="VCC" pad="U5"/>
<connect gate="V2" pin="VCC" pad="AD26"/>
<connect gate="V3" pin="VCC" pad="AF1"/>
<connect gate="V4" pin="VCC" pad="AF26"/>
<connect gate="V5" pin="VCC" pad="A1"/>
<connect gate="V6" pin="VCC" pad="A26"/>
<connect gate="V7" pin="VCC" pad="C14"/>
<connect gate="V8" pin="VCC" pad="C26"/>
<connect gate="V9" pin="VCC" pad="D5"/>
<connect gate="VO1" pin="VCCIO" pad="AB1"/>
<connect gate="VO10" pin="VCCIO" pad="C15"/>
<connect gate="VO11" pin="VCCIO" pad="D25"/>
<connect gate="VO12" pin="VCCIO" pad="F4"/>
<connect gate="VO13" pin="VCCIO" pad="H24"/>
<connect gate="VO14" pin="VCCIO" pad="K5"/>
<connect gate="VO15" pin="VCCIO" pad="M23"/>
<connect gate="VO16" pin="VCCIO" pad="P2"/>
<connect gate="VO17" pin="VCCIO" pad="T25"/>
<connect gate="VO18" pin="VCCIO" pad="V2"/>
<connect gate="VO19" pin="VCCIO" pad="W22"/>
<connect gate="VO2" pin="VCCIO" pad="AC25"/>
<connect gate="VO3" pin="VCCIO" pad="AD18"/>
<connect gate="VO4" pin="VCCIO" pad="AF3"/>
<connect gate="VO5" pin="VCCIO" pad="AF7"/>
<connect gate="VO6" pin="VCCIO" pad="AF16"/>
<connect gate="VO7" pin="VCCIO" pad="A7"/>
<connect gate="VO8" pin="VCCIO" pad="A23"/>
<connect gate="VO9" pin="VCCIO" pad="B4"/>
<connect gate="_" pin="/CE" pad="AC2"/>
<connect gate="_" pin="/CEO" pad="AC22"/>
<connect gate="_" pin="/CONFIG" pad="D2"/>
<connect gate="_" pin="/STATUS" pad="D24"/>
<connect gate="_" pin="CONF_DONE" pad="AC24"/>
<connect gate="_" pin="DATA0" pad="AD3"/>
<connect gate="_" pin="DCLK" pad="AC5"/>
<connect gate="_" pin="GCLK0" pad="A14"/>
<connect gate="_" pin="GCLK1" pad="AF13"/>
<connect gate="_" pin="IN0" pad="B14"/>
<connect gate="_" pin="IN1" pad="A13"/>
<connect gate="_" pin="IN2" pad="AE13"/>
<connect gate="_" pin="IN3" pad="AF14"/>
<connect gate="_" pin="MSEL0" pad="D4"/>
<connect gate="_" pin="MSEL1" pad="D3"/>
<connect gate="_" pin="TCK" pad="AD25"/>
<connect gate="_" pin="TDI" pad="AC3"/>
<connect gate="_" pin="TDO" pad="AC23"/>
<connect gate="_" pin="TMS" pad="D22"/>
<connect gate="_" pin="TRST" pad="D23"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF10K30ABC356-2"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="51R8936"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM7256-Q208" prefix="IC">
<description>&lt;b&gt;EPM7256S&lt;/b&gt;&lt;p&gt;
MAX 7000 family</description>
<gates>
<gate name="_" symbol="7256_208"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="G13" symbol="GND"/>
<gate name="G14" symbol="GND"/>
<gate name="V1" symbol="VCCINT"/>
<gate name="V2" symbol="VCCINT"/>
<gate name="V3" symbol="VCCINT"/>
<gate name="V4" symbol="VCCINT"/>
<gate name="VO1" symbol="VCCIO"/>
<gate name="VO2" symbol="VCCIO"/>
<gate name="VO3" symbol="VCCIO"/>
<gate name="VO4" symbol="VCCIO"/>
<gate name="VO5" symbol="VCCIO"/>
<gate name="VO6" symbol="VCCIO"/>
<gate name="VO7" symbol="VCCIO"/>
<gate name="VO8" symbol="VCCIO"/>
<gate name="VO9" symbol="VCCIO"/>
<gate name="VO10" symbol="VCCIO"/>
<gate name="NC1" symbol="NC"/>
<gate name="NC2" symbol="NC"/>
<gate name="NC3" symbol="NC"/>
<gate name="NC4" symbol="NC"/>
<gate name="NC5" symbol="NC"/>
<gate name="NC6" symbol="NC"/>
<gate name="NC7" symbol="NC"/>
<gate name="NC8" symbol="NC"/>
<gate name="NC9" symbol="NC"/>
<gate name="NC10" symbol="NC"/>
<gate name="NC11" symbol="NC"/>
<gate name="NC12" symbol="NC"/>
<gate name="NC13" symbol="NC"/>
<gate name="NC14" symbol="NC"/>
<gate name="NC15" symbol="NC"/>
<gate name="NC16" symbol="NC"/>
</gates>
<devices>
<device name="" package="RQFP208">
<connects>
<connect gate="G1" pin="GND" pad="14"/>
<connect gate="G10" pin="GND" pad="152"/>
<connect gate="G11" pin="GND" pad="174"/>
<connect gate="G12" pin="GND" pad="180"/>
<connect gate="G13" pin="GND" pad="185"/>
<connect gate="G14" pin="GND" pad="200"/>
<connect gate="G2" pin="GND" pad="32"/>
<connect gate="G3" pin="GND" pad="50"/>
<connect gate="G4" pin="GND" pad="72"/>
<connect gate="G5" pin="GND" pad="75"/>
<connect gate="G6" pin="GND" pad="82"/>
<connect gate="G7" pin="GND" pad="94"/>
<connect gate="G8" pin="GND" pad="116"/>
<connect gate="G9" pin="GND" pad="134"/>
<connect gate="NC1" pin="NC" pad="1"/>
<connect gate="NC10" pin="NC" pad="106"/>
<connect gate="NC11" pin="NC" pad="155"/>
<connect gate="NC12" pin="NC" pad="156"/>
<connect gate="NC13" pin="NC" pad="157"/>
<connect gate="NC14" pin="NC" pad="158"/>
<connect gate="NC15" pin="NC" pad="207"/>
<connect gate="NC16" pin="NC" pad="208"/>
<connect gate="NC2" pin="NC" pad="2"/>
<connect gate="NC3" pin="NC" pad="51"/>
<connect gate="NC4" pin="NC" pad="52"/>
<connect gate="NC5" pin="NC" pad="53"/>
<connect gate="NC6" pin="NC" pad="54"/>
<connect gate="NC7" pin="NC" pad="103"/>
<connect gate="NC8" pin="NC" pad="104"/>
<connect gate="NC9" pin="NC" pad="105"/>
<connect gate="V1" pin="VCC" pad="74"/>
<connect gate="V2" pin="VCC" pad="83"/>
<connect gate="V3" pin="VCC" pad="179"/>
<connect gate="V4" pin="VCC" pad="186"/>
<connect gate="VO1" pin="VCCIO" pad="5"/>
<connect gate="VO10" pin="VCCIO" pad="191"/>
<connect gate="VO2" pin="VCCIO" pad="23"/>
<connect gate="VO3" pin="VCCIO" pad="41"/>
<connect gate="VO4" pin="VCCIO" pad="63"/>
<connect gate="VO5" pin="VCCIO" pad="85"/>
<connect gate="VO6" pin="VCCIO" pad="107"/>
<connect gate="VO7" pin="VCCIO" pad="125"/>
<connect gate="VO8" pin="VCCIO" pad="143"/>
<connect gate="VO9" pin="VCCIO" pad="165"/>
<connect gate="_" pin="GCLK1" pad="184"/>
<connect gate="_" pin="GCLR/" pad="182"/>
<connect gate="_" pin="IO1" pad="153"/>
<connect gate="_" pin="IO101" pad="121"/>
<connect gate="_" pin="IO102" pad="122"/>
<connect gate="_" pin="IO104" pad="123"/>
<connect gate="_" pin="IO105" pad="124"/>
<connect gate="_" pin="IO107" pad="126"/>
<connect gate="_" pin="IO109-TMS" pad="127"/>
<connect gate="_" pin="IO11" pad="163"/>
<connect gate="_" pin="IO110" pad="128"/>
<connect gate="_" pin="IO112" pad="129"/>
<connect gate="_" pin="IO113" pad="79"/>
<connect gate="_" pin="IO115" pad="80"/>
<connect gate="_" pin="IO117" pad="81"/>
<connect gate="_" pin="IO118" pad="84"/>
<connect gate="_" pin="IO120" pad="86"/>
<connect gate="_" pin="IO121" pad="87"/>
<connect gate="_" pin="IO123" pad="88"/>
<connect gate="_" pin="IO125" pad="89"/>
<connect gate="_" pin="IO126" pad="90"/>
<connect gate="_" pin="IO128" pad="91"/>
<connect gate="_" pin="IO129" pad="197"/>
<connect gate="_" pin="IO13" pad="164"/>
<connect gate="_" pin="IO131" pad="196"/>
<connect gate="_" pin="IO133" pad="195"/>
<connect gate="_" pin="IO134" pad="194"/>
<connect gate="_" pin="IO136" pad="193"/>
<connect gate="_" pin="IO137" pad="192"/>
<connect gate="_" pin="IO139" pad="190"/>
<connect gate="_" pin="IO14" pad="166"/>
<connect gate="_" pin="IO142" pad="188"/>
<connect gate="_" pin="IO144" pad="187"/>
<connect gate="_" pin="IO145" pad="27"/>
<connect gate="_" pin="IO147" pad="26"/>
<connect gate="_" pin="IO149" pad="25"/>
<connect gate="_" pin="IO150" pad="24"/>
<connect gate="_" pin="IO152" pad="22"/>
<connect gate="_" pin="IO153" pad="21"/>
<connect gate="_" pin="IO155" pad="20"/>
<connect gate="_" pin="IO157" pad="19"/>
<connect gate="_" pin="IO158" pad="18"/>
<connect gate="_" pin="IO16" pad="167"/>
<connect gate="_" pin="IO160" pad="17"/>
<connect gate="_" pin="IO161" pad="38"/>
<connect gate="_" pin="IO163" pad="37"/>
<connect gate="_" pin="IO165" pad="36"/>
<connect gate="_" pin="IO166" pad="35"/>
<connect gate="_" pin="IO168" pad="34"/>
<connect gate="_" pin="IO169" pad="33"/>
<connect gate="_" pin="IO17" pad="141"/>
<connect gate="_" pin="IO171" pad="31"/>
<connect gate="_" pin="IO174" pad="29"/>
<connect gate="_" pin="IO176" pad="28"/>
<connect gate="_" pin="IO177" pad="66"/>
<connect gate="_" pin="IO179" pad="67"/>
<connect gate="_" pin="IO181" pad="68"/>
<connect gate="_" pin="IO182" pad="69"/>
<connect gate="_" pin="IO184" pad="70"/>
<connect gate="_" pin="IO185" pad="71"/>
<connect gate="_" pin="IO187" pad="73"/>
<connect gate="_" pin="IO189" pad="76"/>
<connect gate="_" pin="IO19" pad="142"/>
<connect gate="_" pin="IO190" pad="77"/>
<connect gate="_" pin="IO192" pad="78"/>
<connect gate="_" pin="IO193" pad="4"/>
<connect gate="_" pin="IO195" pad="3"/>
<connect gate="_" pin="IO197" pad="206"/>
<connect gate="_" pin="IO198" pad="205"/>
<connect gate="_" pin="IO200" pad="204"/>
<connect gate="_" pin="IO201" pad="203"/>
<connect gate="_" pin="IO203" pad="202"/>
<connect gate="_" pin="IO205" pad="201"/>
<connect gate="_" pin="IO206" pad="199"/>
<connect gate="_" pin="IO208" pad="198"/>
<connect gate="_" pin="IO209" pad="16"/>
<connect gate="_" pin="IO21" pad="144"/>
<connect gate="_" pin="IO211" pad="15"/>
<connect gate="_" pin="IO213" pad="13"/>
<connect gate="_" pin="IO214" pad="12"/>
<connect gate="_" pin="IO216" pad="11"/>
<connect gate="_" pin="IO217" pad="10"/>
<connect gate="_" pin="IO219" pad="9"/>
<connect gate="_" pin="IO22" pad="145"/>
<connect gate="_" pin="IO221" pad="8"/>
<connect gate="_" pin="IO222" pad="7"/>
<connect gate="_" pin="IO224" pad="6"/>
<connect gate="_" pin="IO225" pad="49"/>
<connect gate="_" pin="IO227" pad="48"/>
<connect gate="_" pin="IO229" pad="47"/>
<connect gate="_" pin="IO230" pad="46"/>
<connect gate="_" pin="IO232" pad="45"/>
<connect gate="_" pin="IO233" pad="44"/>
<connect gate="_" pin="IO235" pad="43"/>
<connect gate="_" pin="IO237" pad="42"/>
<connect gate="_" pin="IO238" pad="40"/>
<connect gate="_" pin="IO24" pad="146"/>
<connect gate="_" pin="IO240" pad="39"/>
<connect gate="_" pin="IO241" pad="65"/>
<connect gate="_" pin="IO243" pad="64"/>
<connect gate="_" pin="IO245" pad="62"/>
<connect gate="_" pin="IO246" pad="61"/>
<connect gate="_" pin="IO248" pad="60"/>
<connect gate="_" pin="IO249" pad="59"/>
<connect gate="_" pin="IO25" pad="147"/>
<connect gate="_" pin="IO251" pad="58"/>
<connect gate="_" pin="IO253" pad="57"/>
<connect gate="_" pin="IO254" pad="56"/>
<connect gate="_" pin="IO256" pad="55"/>
<connect gate="_" pin="IO27" pad="148"/>
<connect gate="_" pin="IO29" pad="149"/>
<connect gate="_" pin="IO3" pad="154"/>
<connect gate="_" pin="IO30" pad="150"/>
<connect gate="_" pin="IO32" pad="151"/>
<connect gate="_" pin="IO33" pad="108"/>
<connect gate="_" pin="IO35" pad="109"/>
<connect gate="_" pin="IO37" pad="110"/>
<connect gate="_" pin="IO38" pad="111"/>
<connect gate="_" pin="IO40" pad="112"/>
<connect gate="_" pin="IO41" pad="113"/>
<connect gate="_" pin="IO43" pad="114"/>
<connect gate="_" pin="IO45" pad="115"/>
<connect gate="_" pin="IO46" pad="117"/>
<connect gate="_" pin="IO48" pad="118"/>
<connect gate="_" pin="IO49" pad="92"/>
<connect gate="_" pin="IO5" pad="159"/>
<connect gate="_" pin="IO51" pad="93"/>
<connect gate="_" pin="IO53" pad="95"/>
<connect gate="_" pin="IO54" pad="96"/>
<connect gate="_" pin="IO56" pad="97"/>
<connect gate="_" pin="IO57" pad="98"/>
<connect gate="_" pin="IO59" pad="99"/>
<connect gate="_" pin="IO6" pad="160"/>
<connect gate="_" pin="IO61" pad="100"/>
<connect gate="_" pin="IO62" pad="101"/>
<connect gate="_" pin="IO64" pad="102"/>
<connect gate="_" pin="IO65" pad="168"/>
<connect gate="_" pin="IO67" pad="169"/>
<connect gate="_" pin="IO69" pad="170"/>
<connect gate="_" pin="IO70" pad="171"/>
<connect gate="_" pin="IO72" pad="172"/>
<connect gate="_" pin="IO73" pad="173"/>
<connect gate="_" pin="IO75" pad="175"/>
<connect gate="_" pin="IO77-TDI" pad="176"/>
<connect gate="_" pin="IO78" pad="177"/>
<connect gate="_" pin="IO8" pad="161"/>
<connect gate="_" pin="IO80" pad="178"/>
<connect gate="_" pin="IO81" pad="130"/>
<connect gate="_" pin="IO83" pad="131"/>
<connect gate="_" pin="IO85" pad="132"/>
<connect gate="_" pin="IO86" pad="133"/>
<connect gate="_" pin="IO88" pad="135"/>
<connect gate="_" pin="IO89" pad="136"/>
<connect gate="_" pin="IO9" pad="162"/>
<connect gate="_" pin="IO91" pad="137"/>
<connect gate="_" pin="IO93" pad="138"/>
<connect gate="_" pin="IO94" pad="139"/>
<connect gate="_" pin="IO96" pad="140"/>
<connect gate="_" pin="IO97" pad="119"/>
<connect gate="_" pin="IO99" pad="120"/>
<connect gate="_" pin="OE1" pad="183"/>
<connect gate="_" pin="OE2-GCLK2" pad="181"/>
<connect gate="_" pin="TCK-IO173" pad="30"/>
<connect gate="_" pin="TDO-IO141" pad="189"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM7256AEQC208-10N"/>
<attribute name="OC_FARNELL" value="1549440"/>
<attribute name="OC_NEWARK" value="51R9842"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPF6016-P208" prefix="IC">
<description>&lt;b&gt;EPF6016&lt;/b&gt;&lt;p&gt;
FLEX 6000 family</description>
<gates>
<gate name="_" symbol="6016CONT"/>
<gate name="7" symbol="VCCIO"/>
<gate name="8" symbol="VCCIO"/>
<gate name="9" symbol="VCCIO"/>
<gate name="10" symbol="VCCIO"/>
<gate name="11" symbol="VCCIO"/>
<gate name="12" symbol="VCCIO"/>
<gate name="13" symbol="VCCIO"/>
<gate name="14" symbol="VCCIO"/>
<gate name="15" symbol="VCCIO"/>
<gate name="16" symbol="VCCIO"/>
<gate name="17" symbol="VCCIO"/>
<gate name="18" symbol="VCCIO"/>
<gate name="G1" symbol="GND"/>
<gate name="G2" symbol="GND"/>
<gate name="G3" symbol="GND"/>
<gate name="G4" symbol="GND"/>
<gate name="G5" symbol="GND"/>
<gate name="G6" symbol="GND"/>
<gate name="G7" symbol="GND"/>
<gate name="G8" symbol="GND"/>
<gate name="G9" symbol="GND"/>
<gate name="G10" symbol="GND"/>
<gate name="G11" symbol="GND"/>
<gate name="G12" symbol="GND"/>
<gate name="-A" symbol="A15-18"/>
<gate name="-C" symbol="C16-18"/>
<gate name="-D" symbol="D16-18"/>
<gate name="-E" symbol="E16-19"/>
<gate name="-F" symbol="F16-19"/>
<gate name="-G" symbol="IO54-2"/>
<gate name="-H" symbol="IO94-3"/>
<gate name="-I" symbol="IO134-3"/>
<gate name="-J" symbol="IO174-2"/>
<gate name="-K" symbol="IO222-2"/>
<gate name="-B" symbol="B16-19"/>
<gate name="1" symbol="VCCINT"/>
<gate name="2" symbol="VCCINT"/>
<gate name="3" symbol="VCCINT"/>
<gate name="4" symbol="VCCINT"/>
<gate name="5" symbol="VCCINT"/>
<gate name="6" symbol="VCCINT"/>
</gates>
<devices>
<device name="" package="PQFP208">
<connects>
<connect gate="-A" pin="IOA1" pad="1"/>
<connect gate="-A" pin="IOA11" pad="157"/>
<connect gate="-A" pin="IOA12" pad="158"/>
<connect gate="-A" pin="IOA13" pad="159"/>
<connect gate="-A" pin="IOA14" pad="160"/>
<connect gate="-A" pin="IOA15" pad="205"/>
<connect gate="-A" pin="IOA16" pad="206"/>
<connect gate="-A" pin="IOA17" pad="207"/>
<connect gate="-A" pin="IOA18" pad="208"/>
<connect gate="-A" pin="IOA3" pad="2"/>
<connect gate="-A" pin="IOA4" pad="3"/>
<connect gate="-A" pin="IOA6" pad="153"/>
<connect gate="-A" pin="IOA7" pad="154"/>
<connect gate="-A" pin="IOA8" pad="155"/>
<connect gate="-A" pin="IOA9" pad="156"/>
<connect gate="-B" pin="IOB1" pad="4"/>
<connect gate="-B" pin="IOB10" pad="141"/>
<connect gate="-B" pin="IOB11" pad="142"/>
<connect gate="-B" pin="IOB12" pad="143"/>
<connect gate="-B" pin="IOB14" pad="144"/>
<connect gate="-B" pin="IOB15" pad="145"/>
<connect gate="-B" pin="IOB16" pad="146"/>
<connect gate="-B" pin="IOB17" pad="151"/>
<connect gate="-B" pin="IOB18" pad="152"/>
<connect gate="-B" pin="IOB2" pad="5"/>
<connect gate="-B" pin="IOB4" pad="10"/>
<connect gate="-B" pin="IOB5" pad="11"/>
<connect gate="-B" pin="IOB6" pad="12"/>
<connect gate="-B" pin="IOB7" pad="13"/>
<connect gate="-B" pin="IOB8" pad="14"/>
<connect gate="-B" pin="IOB9" pad="15"/>
<connect gate="-C" pin="IOC1" pad="16"/>
<connect gate="-C" pin="IOC10" pad="133"/>
<connect gate="-C" pin="IOC11" pad="134"/>
<connect gate="-C" pin="IOC12" pad="135"/>
<connect gate="-C" pin="IOC13" pad="136"/>
<connect gate="-C" pin="IOC14" pad="137"/>
<connect gate="-C" pin="IOC16" pad="138"/>
<connect gate="-C" pin="IOC17" pad="139"/>
<connect gate="-C" pin="IOC18" pad="140"/>
<connect gate="-C" pin="IOC2" pad="17"/>
<connect gate="-C" pin="IOC3" pad="18"/>
<connect gate="-C" pin="IOC4" pad="19"/>
<connect gate="-C" pin="IOC5" pad="20"/>
<connect gate="-C" pin="IOC6" pad="21"/>
<connect gate="-C" pin="IOC7" pad="22"/>
<connect gate="-C" pin="IOC8" pad="23"/>
<connect gate="-D" pin="IOD1" pad="29"/>
<connect gate="-D" pin="IOD11" pad="120"/>
<connect gate="-D" pin="IOD12" pad="121"/>
<connect gate="-D" pin="IOD13" pad="122"/>
<connect gate="-D" pin="IOD14" pad="123"/>
<connect gate="-D" pin="IOD15" pad="124"/>
<connect gate="-D" pin="IOD16" pad="125"/>
<connect gate="-D" pin="IOD17" pad="126"/>
<connect gate="-D" pin="IOD18" pad="127"/>
<connect gate="-D" pin="IOD3" pad="30"/>
<connect gate="-D" pin="IOD4" pad="31"/>
<connect gate="-D" pin="IOD5" pad="32"/>
<connect gate="-D" pin="IOD6" pad="33"/>
<connect gate="-D" pin="IOD7" pad="34"/>
<connect gate="-D" pin="IOD8" pad="35"/>
<connect gate="-D" pin="IOD9" pad="36"/>
<connect gate="-E" pin="IOE11" pad="108"/>
<connect gate="-E" pin="IOE12" pad="109"/>
<connect gate="-E" pin="IOE13" pad="113"/>
<connect gate="-E" pin="IOE14" pad="114"/>
<connect gate="-E" pin="IOE15" pad="115"/>
<connect gate="-E" pin="IOE16" pad="116"/>
<connect gate="-E" pin="IOE17" pad="117"/>
<connect gate="-E" pin="IOE18" pad="118"/>
<connect gate="-E" pin="IOE19" pad="119"/>
<connect gate="-E" pin="IOE2" pad="37"/>
<connect gate="-E" pin="IOE3" pad="38"/>
<connect gate="-E" pin="IOE4" pad="39"/>
<connect gate="-E" pin="IOE5" pad="40"/>
<connect gate="-E" pin="IOE6" pad="41"/>
<connect gate="-E" pin="IOE7" pad="42"/>
<connect gate="-E" pin="IOE9" pad="47"/>
<connect gate="-F" pin="IOF1" pad="48"/>
<connect gate="-F" pin="IOF10" pad="56"/>
<connect gate="-F" pin="IOF11" pad="101"/>
<connect gate="-F" pin="IOF12" pad="102"/>
<connect gate="-F" pin="IOF13" pad="103"/>
<connect gate="-F" pin="IOF14" pad="104"/>
<connect gate="-F" pin="IOF15" pad="105"/>
<connect gate="-F" pin="IOF17" pad="106"/>
<connect gate="-F" pin="IOF18" pad="107"/>
<connect gate="-F" pin="IOF2" pad="49"/>
<connect gate="-F" pin="IOF3" pad="50"/>
<connect gate="-F" pin="IOF4" pad="51"/>
<connect gate="-F" pin="IOF5" pad="52"/>
<connect gate="-F" pin="IOF7" pad="53"/>
<connect gate="-F" pin="IOF8" pad="54"/>
<connect gate="-F" pin="IOF9" pad="55"/>
<connect gate="-G" pin="IO11" pad="57"/>
<connect gate="-G" pin="IO12" pad="204"/>
<connect gate="-G" pin="IO21" pad="58"/>
<connect gate="-G" pin="IO22" pad="59"/>
<connect gate="-G" pin="IO23" pad="202"/>
<connect gate="-G" pin="IO24" pad="203"/>
<connect gate="-G" pin="IO31" pad="60"/>
<connect gate="-G" pin="IO32" pad="61"/>
<connect gate="-G" pin="IO34" pad="201"/>
<connect gate="-G" pin="IO41" pad="64"/>
<connect gate="-G" pin="IO43" pad="197"/>
<connect gate="-G" pin="IO44" pad="198"/>
<connect gate="-G" pin="IO51" pad="65"/>
<connect gate="-G" pin="IO52" pad="66"/>
<connect gate="-G" pin="IO53" pad="195"/>
<connect gate="-G" pin="IO54" pad="196"/>
<connect gate="-H" pin="IO61" pad="67"/>
<connect gate="-H" pin="IO63" pad="193"/>
<connect gate="-H" pin="IO64" pad="194"/>
<connect gate="-H" pin="IO71" pad="68"/>
<connect gate="-H" pin="IO72" pad="69"/>
<connect gate="-H" pin="IO73" pad="191"/>
<connect gate="-H" pin="IO74" pad="192"/>
<connect gate="-H" pin="IO81" pad="70"/>
<connect gate="-H" pin="IO82" pad="71"/>
<connect gate="-H" pin="IO83" pad="190"/>
<connect gate="-H" pin="IO91" pad="72"/>
<connect gate="-H" pin="IO93" pad="188"/>
<connect gate="-H" pin="IO94" pad="189"/>
<connect gate="-I" pin="IO101" pad="73"/>
<connect gate="-I" pin="IO102" pad="74"/>
<connect gate="-I" pin="IO104" pad="187"/>
<connect gate="-I" pin="IO111" pad="75"/>
<connect gate="-I" pin="IO112" pad="76"/>
<connect gate="-I" pin="IO113" pad="185"/>
<connect gate="-I" pin="IO114" pad="186"/>
<connect gate="-I" pin="IO121" pad="81"/>
<connect gate="-I" pin="IO122" pad="82"/>
<connect gate="-I" pin="IO123" pad="180"/>
<connect gate="-I" pin="IO132" pad="83"/>
<connect gate="-I" pin="IO133" pad="178"/>
<connect gate="-I" pin="IO134" pad="179"/>
<connect gate="-J" pin="IO141" pad="84"/>
<connect gate="-J" pin="IO142" pad="85"/>
<connect gate="-J" pin="IO143" pad="177"/>
<connect gate="-J" pin="IO151" pad="86"/>
<connect gate="-J" pin="IO152" pad="87"/>
<connect gate="-J" pin="IO153" pad="175"/>
<connect gate="-J" pin="IO154" pad="176"/>
<connect gate="-J" pin="IO161" pad="88"/>
<connect gate="-J" pin="IO162" pad="89"/>
<connect gate="-J" pin="IO163" pad="173"/>
<connect gate="-J" pin="IO164" pad="174"/>
<connect gate="-J" pin="IO172" pad="90"/>
<connect gate="-J" pin="IO173" pad="171"/>
<connect gate="-J" pin="IO174" pad="172"/>
<connect gate="-K" pin="IO181" pad="91"/>
<connect gate="-K" pin="IO182" pad="92"/>
<connect gate="-K" pin="IO183" pad="169"/>
<connect gate="-K" pin="IO184" pad="170"/>
<connect gate="-K" pin="IO191" pad="93"/>
<connect gate="-K" pin="IO192" pad="94"/>
<connect gate="-K" pin="IO193" pad="167"/>
<connect gate="-K" pin="IO194" pad="168"/>
<connect gate="-K" pin="IO202" pad="97"/>
<connect gate="-K" pin="IO203" pad="163"/>
<connect gate="-K" pin="IO204" pad="164"/>
<connect gate="-K" pin="IO211" pad="98"/>
<connect gate="-K" pin="IO212" pad="99"/>
<connect gate="-K" pin="IO214" pad="162"/>
<connect gate="-K" pin="IO221" pad="100"/>
<connect gate="-K" pin="IO222" pad="161"/>
<connect gate="1" pin="VCC" pad="8"/>
<connect gate="10" pin="VCCIO" pad="63"/>
<connect gate="11" pin="VCCIO" pad="79"/>
<connect gate="12" pin="VCCIO" pad="96"/>
<connect gate="13" pin="VCCIO" pad="112"/>
<connect gate="14" pin="VCCIO" pad="131"/>
<connect gate="15" pin="VCCIO" pad="149"/>
<connect gate="16" pin="VCCIO" pad="166"/>
<connect gate="17" pin="VCCIO" pad="183"/>
<connect gate="18" pin="VCCIO" pad="200"/>
<connect gate="2" pin="VCC" pad="26"/>
<connect gate="3" pin="VCC" pad="44"/>
<connect gate="4" pin="VCC" pad="111"/>
<connect gate="5" pin="VCC" pad="130"/>
<connect gate="6" pin="VCC" pad="148"/>
<connect gate="7" pin="VCCIO" pad="9"/>
<connect gate="8" pin="VCCIO" pad="27"/>
<connect gate="9" pin="VCCIO" pad="45"/>
<connect gate="G1" pin="GND" pad="7"/>
<connect gate="G10" pin="GND" pad="165"/>
<connect gate="G11" pin="GND" pad="182"/>
<connect gate="G12" pin="GND" pad="199"/>
<connect gate="G2" pin="GND" pad="25"/>
<connect gate="G3" pin="GND" pad="43"/>
<connect gate="G4" pin="GND" pad="62"/>
<connect gate="G5" pin="GND" pad="78"/>
<connect gate="G6" pin="GND" pad="95"/>
<connect gate="G7" pin="GND" pad="110"/>
<connect gate="G8" pin="GND" pad="129"/>
<connect gate="G9" pin="GND" pad="147"/>
<connect gate="_" pin="!CE" pad="6"/>
<connect gate="_" pin="!CONFIG" pad="77"/>
<connect gate="_" pin="!STATUS" pad="80"/>
<connect gate="_" pin="CONF_DONE" pad="150"/>
<connect gate="_" pin="DATA0" pad="181"/>
<connect gate="_" pin="DCLK" pad="184"/>
<connect gate="_" pin="GCLK1" pad="24"/>
<connect gate="_" pin="GCLK2" pad="28"/>
<connect gate="_" pin="GCLK3" pad="128"/>
<connect gate="_" pin="GCLK4" pad="132"/>
<connect gate="_" pin="MSEL" pad="46"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPF6016AQC208-3N"/>
<attribute name="OC_FARNELL" value="1549398"/>
<attribute name="OC_NEWARK" value="51R9156"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240T100C4" prefix="IC">
<description>&lt;b&gt;EPM240T100&lt;/b&gt; Low-cost, low-power CPLD&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 35&lt;/i&gt;&lt;br&gt;
Source: www.altera.com .. epm240-io.txt</description>
<gates>
<gate name="G$1" symbol="EPM240T100C4"/>
</gates>
<devices>
<device name="" package="TQFP100">
<connects>
<connect gate="G$1" pin="B1/0" pad="2"/>
<connect gate="G$1" pin="B1/1" pad="3"/>
<connect gate="G$1" pin="B1/10-GCLK0" pad="12"/>
<connect gate="G$1" pin="B1/12-GCLK1" pad="14"/>
<connect gate="G$1" pin="B1/13" pad="15"/>
<connect gate="G$1" pin="B1/14" pad="16"/>
<connect gate="G$1" pin="B1/15" pad="17"/>
<connect gate="G$1" pin="B1/16" pad="18"/>
<connect gate="G$1" pin="B1/17" pad="19"/>
<connect gate="G$1" pin="B1/18" pad="20"/>
<connect gate="G$1" pin="B1/19" pad="21"/>
<connect gate="G$1" pin="B1/2" pad="4"/>
<connect gate="G$1" pin="B1/20-TMS" pad="22"/>
<connect gate="G$1" pin="B1/21-TDI" pad="23"/>
<connect gate="G$1" pin="B1/22-TCK" pad="24"/>
<connect gate="G$1" pin="B1/24-TDO" pad="25"/>
<connect gate="G$1" pin="B1/25" pad="26"/>
<connect gate="G$1" pin="B1/26" pad="27"/>
<connect gate="G$1" pin="B1/27" pad="28"/>
<connect gate="G$1" pin="B1/28" pad="29"/>
<connect gate="G$1" pin="B1/29" pad="30"/>
<connect gate="G$1" pin="B1/3" pad="5"/>
<connect gate="G$1" pin="B1/32" pad="33"/>
<connect gate="G$1" pin="B1/33" pad="34"/>
<connect gate="G$1" pin="B1/34" pad="35"/>
<connect gate="G$1" pin="B1/35" pad="36"/>
<connect gate="G$1" pin="B1/36" pad="37"/>
<connect gate="G$1" pin="B1/37" pad="38"/>
<connect gate="G$1" pin="B1/38" pad="39"/>
<connect gate="G$1" pin="B1/39" pad="40"/>
<connect gate="G$1" pin="B1/4" pad="6"/>
<connect gate="G$1" pin="B1/40" pad="41"/>
<connect gate="G$1" pin="B1/41" pad="42"/>
<connect gate="G$1" pin="B1/42-DEV_OE" pad="43"/>
<connect gate="G$1" pin="B1/43-DEV_CLRN" pad="44"/>
<connect gate="G$1" pin="B1/46" pad="47"/>
<connect gate="G$1" pin="B1/47" pad="48"/>
<connect gate="G$1" pin="B1/48" pad="49"/>
<connect gate="G$1" pin="B1/49" pad="50"/>
<connect gate="G$1" pin="B1/5" pad="7"/>
<connect gate="G$1" pin="B1/50" pad="51"/>
<connect gate="G$1" pin="B1/6" pad="8"/>
<connect gate="G$1" pin="B2/100" pad="1"/>
<connect gate="G$1" pin="B2/51" pad="52"/>
<connect gate="G$1" pin="B2/52" pad="53"/>
<connect gate="G$1" pin="B2/53" pad="54"/>
<connect gate="G$1" pin="B2/54" pad="55"/>
<connect gate="G$1" pin="B2/55" pad="56"/>
<connect gate="G$1" pin="B2/56" pad="57"/>
<connect gate="G$1" pin="B2/57" pad="58"/>
<connect gate="G$1" pin="B2/60" pad="61"/>
<connect gate="G$1" pin="B2/61-GCLK2" pad="62"/>
<connect gate="G$1" pin="B2/63-GCLK3" pad="64"/>
<connect gate="G$1" pin="B2/65" pad="66"/>
<connect gate="G$1" pin="B2/66" pad="67"/>
<connect gate="G$1" pin="B2/67" pad="68"/>
<connect gate="G$1" pin="B2/68" pad="69"/>
<connect gate="G$1" pin="B2/69" pad="70"/>
<connect gate="G$1" pin="B2/70" pad="71"/>
<connect gate="G$1" pin="B2/71" pad="72"/>
<connect gate="G$1" pin="B2/72" pad="73"/>
<connect gate="G$1" pin="B2/73" pad="74"/>
<connect gate="G$1" pin="B2/74" pad="75"/>
<connect gate="G$1" pin="B2/75" pad="76"/>
<connect gate="G$1" pin="B2/76" pad="77"/>
<connect gate="G$1" pin="B2/77" pad="78"/>
<connect gate="G$1" pin="B2/80" pad="81"/>
<connect gate="G$1" pin="B2/81" pad="82"/>
<connect gate="G$1" pin="B2/82" pad="83"/>
<connect gate="G$1" pin="B2/83" pad="84"/>
<connect gate="G$1" pin="B2/84" pad="85"/>
<connect gate="G$1" pin="B2/85" pad="86"/>
<connect gate="G$1" pin="B2/86" pad="87"/>
<connect gate="G$1" pin="B2/87" pad="88"/>
<connect gate="G$1" pin="B2/88" pad="89"/>
<connect gate="G$1" pin="B2/89" pad="90"/>
<connect gate="G$1" pin="B2/90" pad="91"/>
<connect gate="G$1" pin="B2/91" pad="92"/>
<connect gate="G$1" pin="B2/94" pad="95"/>
<connect gate="G$1" pin="B2/95" pad="96"/>
<connect gate="G$1" pin="B2/96" pad="97"/>
<connect gate="G$1" pin="B2/97" pad="98"/>
<connect gate="G$1" pin="B2/98" pad="99"/>
<connect gate="G$1" pin="B2/99" pad="100"/>
<connect gate="G$1" pin="GNDINT" pad="11"/>
<connect gate="G$1" pin="GNDINT@1" pad="65"/>
<connect gate="G$1" pin="GNDIO" pad="10"/>
<connect gate="G$1" pin="GNDIO@1" pad="32"/>
<connect gate="G$1" pin="GNDIO@2" pad="46"/>
<connect gate="G$1" pin="GNDIO@3" pad="60"/>
<connect gate="G$1" pin="GNDIO@4" pad="79"/>
<connect gate="G$1" pin="GNDIO@5" pad="93"/>
<connect gate="G$1" pin="VCCINT" pad="13"/>
<connect gate="G$1" pin="VCCINT@1" pad="63"/>
<connect gate="G$1" pin="VCCIO" pad="9"/>
<connect gate="G$1" pin="VCCIO@1" pad="31"/>
<connect gate="G$1" pin="VCCIO@2" pad="45"/>
<connect gate="G$1" pin="VCCIO@3" pad="59"/>
<connect gate="G$1" pin="VCCIO@4" pad="80"/>
<connect gate="G$1" pin="VCCIO@5" pad="94"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM240T100C4"/>
<attribute name="OC_FARNELL" value="1453502"/>
<attribute name="OC_NEWARK" value="51R9357"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240F100" prefix="IC">
<description>&lt;b&gt;EPM240F100&lt;/b&gt; &lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 36&lt;/i&gt;&lt;br&gt;
Source: EPM240F100.BSD</description>
<gates>
<gate name="G$1" symbol="EPM240F100"/>
</gates>
<devices>
<device name="" package="FBGA100">
<connects>
<connect gate="G$1" pin="GND@1" pad="E5"/>
<connect gate="G$1" pin="GND@2" pad="F5"/>
<connect gate="G$1" pin="GND@3" pad="G5"/>
<connect gate="G$1" pin="GND@4" pad="G7"/>
<connect gate="G$1" pin="GND@5" pad="F6"/>
<connect gate="G$1" pin="GND@6" pad="E6"/>
<connect gate="G$1" pin="GND@7" pad="D7"/>
<connect gate="G$1" pin="GND@8" pad="D5"/>
<connect gate="G$1" pin="IOA1" pad="A1"/>
<connect gate="G$1" pin="IOA10" pad="A10"/>
<connect gate="G$1" pin="IOA2" pad="A2"/>
<connect gate="G$1" pin="IOA3" pad="A3"/>
<connect gate="G$1" pin="IOA4" pad="A4"/>
<connect gate="G$1" pin="IOA5" pad="A5"/>
<connect gate="G$1" pin="IOA6" pad="A6"/>
<connect gate="G$1" pin="IOA7" pad="A7"/>
<connect gate="G$1" pin="IOA8" pad="A8"/>
<connect gate="G$1" pin="IOA9" pad="A9"/>
<connect gate="G$1" pin="IOB1" pad="B1"/>
<connect gate="G$1" pin="IOB10" pad="B10"/>
<connect gate="G$1" pin="IOB2" pad="B2"/>
<connect gate="G$1" pin="IOB3" pad="B3"/>
<connect gate="G$1" pin="IOB4" pad="B4"/>
<connect gate="G$1" pin="IOB5" pad="B5"/>
<connect gate="G$1" pin="IOB6" pad="B6"/>
<connect gate="G$1" pin="IOB7" pad="B7"/>
<connect gate="G$1" pin="IOB8" pad="B8"/>
<connect gate="G$1" pin="IOB9" pad="B9"/>
<connect gate="G$1" pin="IOC1" pad="C1"/>
<connect gate="G$1" pin="IOC10" pad="C10"/>
<connect gate="G$1" pin="IOC2" pad="C2"/>
<connect gate="G$1" pin="IOC3" pad="C3"/>
<connect gate="G$1" pin="IOC4" pad="C4"/>
<connect gate="G$1" pin="IOC5" pad="C5"/>
<connect gate="G$1" pin="IOC6" pad="C6"/>
<connect gate="G$1" pin="IOC7" pad="C7"/>
<connect gate="G$1" pin="IOC8" pad="C8"/>
<connect gate="G$1" pin="IOC9" pad="C9"/>
<connect gate="G$1" pin="IOD1" pad="D1"/>
<connect gate="G$1" pin="IOD10" pad="D10"/>
<connect gate="G$1" pin="IOD2" pad="D2"/>
<connect gate="G$1" pin="IOD3" pad="D3"/>
<connect gate="G$1" pin="IOD8" pad="D8"/>
<connect gate="G$1" pin="IOD9" pad="D9"/>
<connect gate="G$1" pin="IOE1" pad="E1"/>
<connect gate="G$1" pin="IOE10" pad="E10"/>
<connect gate="G$1" pin="IOE2" pad="E2"/>
<connect gate="G$1" pin="IOE3" pad="E3"/>
<connect gate="G$1" pin="IOE8" pad="E8"/>
<connect gate="G$1" pin="IOE9" pad="E9"/>
<connect gate="G$1" pin="IOF1" pad="F1"/>
<connect gate="G$1" pin="IOF10" pad="F10"/>
<connect gate="G$1" pin="IOF2" pad="F2"/>
<connect gate="G$1" pin="IOF3" pad="F3"/>
<connect gate="G$1" pin="IOF8" pad="F8"/>
<connect gate="G$1" pin="IOF9" pad="F9"/>
<connect gate="G$1" pin="IOG1" pad="G1"/>
<connect gate="G$1" pin="IOG10" pad="G10"/>
<connect gate="G$1" pin="IOG2" pad="G2"/>
<connect gate="G$1" pin="IOG3" pad="G3"/>
<connect gate="G$1" pin="IOG8" pad="G8"/>
<connect gate="G$1" pin="IOG9" pad="G9"/>
<connect gate="G$1" pin="IOH1" pad="H1"/>
<connect gate="G$1" pin="IOH10" pad="H10"/>
<connect gate="G$1" pin="IOH4" pad="H4"/>
<connect gate="G$1" pin="IOH5" pad="H5"/>
<connect gate="G$1" pin="IOH6" pad="H6"/>
<connect gate="G$1" pin="IOH7" pad="H7"/>
<connect gate="G$1" pin="IOH8" pad="H8"/>
<connect gate="G$1" pin="IOH9" pad="H9"/>
<connect gate="G$1" pin="IOJ10" pad="J10"/>
<connect gate="G$1" pin="IOJ3" pad="J3"/>
<connect gate="G$1" pin="IOJ4" pad="J4"/>
<connect gate="G$1" pin="IOJ5" pad="J5"/>
<connect gate="G$1" pin="IOJ6" pad="J6"/>
<connect gate="G$1" pin="IOJ7" pad="J7"/>
<connect gate="G$1" pin="IOJ8" pad="J8"/>
<connect gate="G$1" pin="IOJ9" pad="J9"/>
<connect gate="G$1" pin="IOK1" pad="K1"/>
<connect gate="G$1" pin="IOK10" pad="K10"/>
<connect gate="G$1" pin="IOK2" pad="K2"/>
<connect gate="G$1" pin="IOK3" pad="K3"/>
<connect gate="G$1" pin="IOK4" pad="K4"/>
<connect gate="G$1" pin="IOK5" pad="K5"/>
<connect gate="G$1" pin="IOK6" pad="K6"/>
<connect gate="G$1" pin="IOK7" pad="K7"/>
<connect gate="G$1" pin="IOK8" pad="K8"/>
<connect gate="G$1" pin="IOK9" pad="K9"/>
<connect gate="G$1" pin="TCK" pad="H3"/>
<connect gate="G$1" pin="TDI" pad="H2"/>
<connect gate="G$1" pin="TDO" pad="J2"/>
<connect gate="G$1" pin="TMS" pad="J1"/>
<connect gate="G$1" pin="VCC@1" pad="E4"/>
<connect gate="G$1" pin="VCC@2" pad="F4"/>
<connect gate="G$1" pin="VCC@3" pad="G4"/>
<connect gate="G$1" pin="VCC@4" pad="G6"/>
<connect gate="G$1" pin="VCC@5" pad="F7"/>
<connect gate="G$1" pin="VCC@6" pad="E7"/>
<connect gate="G$1" pin="VCC@7" pad="D6"/>
<connect gate="G$1" pin="VCC@8" pad="D4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SA800-B293"/>
<attribute name="OC_FARNELL" value="1635094"/>
<attribute name="OC_NEWARK" value="74R0178"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EPM240M100" prefix="IC">
<description>&lt;b&gt;EPM240M100&lt;/b&gt; Low-cost, low-power CPLD&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 36&lt;/i&gt;&lt;br&gt;
Source: EPM240M100.BSD</description>
<gates>
<gate name="G$1" symbol="EPM240M100"/>
</gates>
<devices>
<device name="" package="MBGA100">
<connects>
<connect gate="G$1" pin="GND@1" pad="E4"/>
<connect gate="G$1" pin="GND@2" pad="G4"/>
<connect gate="G$1" pin="GND@3" pad="H5"/>
<connect gate="G$1" pin="GND@4" pad="H7"/>
<connect gate="G$1" pin="GND@5" pad="G8"/>
<connect gate="G$1" pin="GND@6" pad="E8"/>
<connect gate="G$1" pin="GND@7" pad="D7"/>
<connect gate="G$1" pin="GND@8" pad="D5"/>
<connect gate="G$1" pin="IOA1" pad="A1"/>
<connect gate="G$1" pin="IOA10" pad="A10"/>
<connect gate="G$1" pin="IOA11" pad="A11"/>
<connect gate="G$1" pin="IOA2" pad="A2"/>
<connect gate="G$1" pin="IOA3" pad="A3"/>
<connect gate="G$1" pin="IOA4" pad="A4"/>
<connect gate="G$1" pin="IOA5" pad="A5"/>
<connect gate="G$1" pin="IOA6" pad="A6"/>
<connect gate="G$1" pin="IOA7" pad="A7"/>
<connect gate="G$1" pin="IOA8" pad="A8"/>
<connect gate="G$1" pin="IOA9" pad="A9"/>
<connect gate="G$1" pin="IOB1" pad="B1"/>
<connect gate="G$1" pin="IOB10" pad="B10"/>
<connect gate="G$1" pin="IOB11" pad="B11"/>
<connect gate="G$1" pin="IOB2" pad="B2"/>
<connect gate="G$1" pin="IOB3" pad="B3"/>
<connect gate="G$1" pin="IOB4" pad="B4"/>
<connect gate="G$1" pin="IOB5" pad="B5"/>
<connect gate="G$1" pin="IOB6" pad="B6"/>
<connect gate="G$1" pin="IOB7" pad="B7"/>
<connect gate="G$1" pin="IOB8" pad="B8"/>
<connect gate="G$1" pin="IOB9" pad="B9"/>
<connect gate="G$1" pin="IOC1" pad="C1"/>
<connect gate="G$1" pin="IOC10" pad="C10"/>
<connect gate="G$1" pin="IOC11" pad="C11"/>
<connect gate="G$1" pin="IOC2" pad="C2"/>
<connect gate="G$1" pin="IOC5" pad="C5"/>
<connect gate="G$1" pin="IOC6" pad="C6"/>
<connect gate="G$1" pin="IOC7" pad="C7"/>
<connect gate="G$1" pin="IOD1" pad="D1"/>
<connect gate="G$1" pin="IOD10" pad="D10"/>
<connect gate="G$1" pin="IOD11" pad="D11"/>
<connect gate="G$1" pin="IOD2" pad="D2"/>
<connect gate="G$1" pin="IOD3" pad="D3"/>
<connect gate="G$1" pin="IOD9" pad="D9"/>
<connect gate="G$1" pin="IOE1" pad="E1"/>
<connect gate="G$1" pin="IOE10" pad="E10"/>
<connect gate="G$1" pin="IOE11" pad="E11"/>
<connect gate="G$1" pin="IOE2" pad="E2"/>
<connect gate="G$1" pin="IOF1" pad="F1"/>
<connect gate="G$1" pin="IOF10" pad="F10"/>
<connect gate="G$1" pin="IOF11" pad="F11"/>
<connect gate="G$1" pin="IOF2" pad="F2"/>
<connect gate="G$1" pin="IOF3" pad="F3"/>
<connect gate="G$1" pin="IOF9" pad="F9"/>
<connect gate="G$1" pin="IOG1" pad="G1"/>
<connect gate="G$1" pin="IOG10" pad="G10"/>
<connect gate="G$1" pin="IOG11" pad="G11"/>
<connect gate="G$1" pin="IOG2" pad="G2"/>
<connect gate="G$1" pin="IOH1" pad="H1"/>
<connect gate="G$1" pin="IOH10" pad="H10"/>
<connect gate="G$1" pin="IOH11" pad="H11"/>
<connect gate="G$1" pin="IOH2" pad="H2"/>
<connect gate="G$1" pin="IOH3" pad="H3"/>
<connect gate="G$1" pin="IOH9" pad="H9"/>
<connect gate="G$1" pin="IOJ10" pad="J10"/>
<connect gate="G$1" pin="IOJ11" pad="J11"/>
<connect gate="G$1" pin="IOJ5" pad="J5"/>
<connect gate="G$1" pin="IOJ6" pad="J6"/>
<connect gate="G$1" pin="IOJ7" pad="J7"/>
<connect gate="G$1" pin="IOK10" pad="K10"/>
<connect gate="G$1" pin="IOK11" pad="K11"/>
<connect gate="G$1" pin="IOK3" pad="K3"/>
<connect gate="G$1" pin="IOK4" pad="K4"/>
<connect gate="G$1" pin="IOK5" pad="K5"/>
<connect gate="G$1" pin="IOK6" pad="K6"/>
<connect gate="G$1" pin="IOK7" pad="K7"/>
<connect gate="G$1" pin="IOK8" pad="K8"/>
<connect gate="G$1" pin="IOK9" pad="K9"/>
<connect gate="G$1" pin="IOL1" pad="L1"/>
<connect gate="G$1" pin="IOL10" pad="L10"/>
<connect gate="G$1" pin="IOL11" pad="L11"/>
<connect gate="G$1" pin="IOL2" pad="L2"/>
<connect gate="G$1" pin="IOL3" pad="L3"/>
<connect gate="G$1" pin="IOL4" pad="L4"/>
<connect gate="G$1" pin="IOL5" pad="L5"/>
<connect gate="G$1" pin="IOL6" pad="L6"/>
<connect gate="G$1" pin="IOL7" pad="L7"/>
<connect gate="G$1" pin="IOL8" pad="L8"/>
<connect gate="G$1" pin="IOL9" pad="L9"/>
<connect gate="G$1" pin="TCK" pad="K1"/>
<connect gate="G$1" pin="TDI" pad="J2"/>
<connect gate="G$1" pin="TDO" pad="K2"/>
<connect gate="G$1" pin="TMS" pad="J1"/>
<connect gate="G$1" pin="VCC@1" pad="E3"/>
<connect gate="G$1" pin="VCC@2" pad="G3"/>
<connect gate="G$1" pin="VCC@3" pad="J4"/>
<connect gate="G$1" pin="VCC@4" pad="J8"/>
<connect gate="G$1" pin="VCC@5" pad="G9"/>
<connect gate="G$1" pin="VCC@6" pad="E9"/>
<connect gate="G$1" pin="VCC@7" pad="C8"/>
<connect gate="G$1" pin="VCC@8" pad="C4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="EPM240M100C4N"/>
<attribute name="OC_FARNELL" value="1635095"/>
<attribute name="OC_NEWARK" value="51R0493"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
