<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;PC Connectors/Slots&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PCI_BRD">
<description>&lt;b&gt;PCI BOARD SHORT&lt;/b&gt;</description>
</package>
<package name="PCI_BRDL">
<description>&lt;b&gt;PCI BOARD LONG&lt;/b&gt;</description>
</package>
<package name="VERO-G44">
<description>&lt;B&gt;SLOT HOLDER&lt;/B&gt;&lt;p&gt;
VERO</description>
</package>
<package name="IBM16BIT">
<description>&lt;B&gt;16-bit CARD IBM/PC-AT&lt;/B&gt;</description>
</package>
<package name="IBM8BIT">
<description>&lt;B&gt;8-bit CARD IBM/PC-AT&lt;/B&gt;</description>
</package>
<package name="IBM_8AB">
<description>&lt;B&gt;8-bit CARD IBM/PC-AT&lt;/B&gt;</description>
</package>
<package name="ISA-16">
<description>&lt;B&gt;ISA SLOT&lt;/B&gt;</description>
</package>
<package name="CON-PCI">
<description>&lt;B&gt;PCI SLOT&lt;/B&gt;</description>
</package>
<package name="EISA-188">
<description>&lt;B&gt;EISA SLOT&lt;/B&gt;</description>
</package>
<package name="EISA-BRD">
<description>&lt;b&gt;EISA CARD CONNECTOR&lt;/b&gt;</description>
</package>
<package name="PCI-LONG">
<description>&lt;b&gt;PCI BOARD LONG&lt;/b&gt;</description>
</package>
<package name="SC242CON">
<description>&lt;B&gt;SLOT1 CONNECTOR&lt;/B&gt;&lt;p&gt;
Intel</description>
</package>
<package name="AGP">
<description>&lt;b&gt;AGP Slot&lt;/b&gt; AMP connctor 145263 &amp;gt;PCT-GF40&amp;lt;&lt;p&gt;
124 Position 1mm, card edge connector&lt;br&gt;
Drawing No: C-145263&lt;br&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_145263_H.pdf</description>
</package>
<package name="AGP_UC">
<description>&lt;b&gt;AGP:UC Slot&lt;/b&gt; AMP connctor 145376 &amp;gt;PCT-GF40&amp;lt; &lt;p&gt;
132 Position 1mm, card edge connector&lt;br&gt;
Drawing No: C-145263&lt;br&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_145376_D.pdf</description>
</package>
<package name="AGP-SLOT">
<description>&lt;b&gt;AGP&lt;/b&gt; 124 Position 1mm Card Edge connector&lt;p&gt;
Drawing No: C-145263&lt;br&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_145263_H.pdf</description>
</package>
<package name="AGP_UC-SLOT">
<description>&lt;b&gt;AGP:UC&lt;/b&gt; 132 Position 1mm Card connector&lt;p&gt;
Drawing No: C-145376&lt;br&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_145376_D.pdf</description>
</package>
<package name="PCI-E_SLOT">
<description>Copy from  &lt;b&gt;con-pci_express(pci-e).lbr&lt;/b&gt; uploaded &lt;i&gt;Mon Jul 2 10:15:25 2007&lt;/i&gt; with Finished-Layer&lt;p&gt; 
Library for PCI-Express x16 (PCI-E) connector. Includes connector and card edge pattern.&lt;br&gt;
Uploaded by JF Duval &amp;lt;jfduval@aqra.ca&amp;gt; from AQRA.ca</description>
</package>
<package name="PCI-E-164">
<description>Copy from  &lt;b&gt;con-pci_express(pci-e).lbr&lt;/b&gt; uploaded &lt;i&gt;Mon Jul 2 10:15:25 2007&lt;/i&gt;&lt;p&gt; 
Library for PCI-Express x16 (PCI-E) connector. Includes connector and card edge pattern.&lt;br&gt;
Uploaded by JF Duval &amp;lt;jfduval@aqra.ca&amp;gt; from AQRA.ca</description>
</package>
</packages>
<symbols>
<symbol name="PCI_CON">
<pin name="/ACK64" direction="pas"/>
<pin name="/DEVSEL" direction="pas"/>
<pin name="/FRAME" direction="pas"/>
<pin name="/GNT" direction="pas"/>
<pin name="/INTA" direction="pas"/>
<pin name="/INTB" direction="pas"/>
<pin name="/INTC" direction="pas"/>
<pin name="/INTD" direction="pas"/>
<pin name="/IRDY" direction="pas"/>
<pin name="/LOCK" direction="pas"/>
<pin name="/PERR" direction="pas"/>
<pin name="/PRSNT1" direction="pas"/>
<pin name="/PRSNT2" direction="pas"/>
<pin name="/REQ" direction="pas"/>
<pin name="/REQ64" direction="pas"/>
<pin name="/RST" direction="pas"/>
<pin name="/SBO" direction="pas"/>
<pin name="/SERR" direction="pas"/>
<pin name="/STOP" direction="pas"/>
<pin name="/TRDY" direction="pas"/>
<pin name="/TRST" direction="pas"/>
<pin name="+3,3V" direction="pwr"/>
<pin name="+3,3V@1" direction="pwr"/>
<pin name="+3,3V@2" direction="pwr"/>
<pin name="+3,3V@3" direction="pas"/>
<pin name="+3,3V@4" direction="pwr"/>
<pin name="+3,3V@5" direction="pwr"/>
<pin name="+3,3V@11" direction="pwr"/>
<pin name="+3,3V@10" direction="pwr"/>
<pin name="+3,3V@9" direction="pwr"/>
<pin name="+3,3V@8" direction="pwr"/>
<pin name="+3,3V@7" direction="pwr"/>
<pin name="+3,3V@6" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
<pin name="+5V@1" direction="pwr"/>
<pin name="+5V@2" direction="pwr"/>
<pin name="+5V@3" direction="pwr"/>
<pin name="+5V@4" direction="pwr"/>
<pin name="+5V@5" direction="pwr"/>
<pin name="+5V@6" direction="pwr"/>
<pin name="+5V@12" direction="pwr"/>
<pin name="+5V@11" direction="pwr"/>
<pin name="+5V@10" direction="pwr"/>
<pin name="+5V@9" direction="pwr"/>
<pin name="+5V@8" direction="pwr"/>
<pin name="+5V@7" direction="pwr"/>
<pin name="+12V" direction="pwr"/>
<pin name="-12V" direction="pwr"/>
<pin name="AD0" direction="pas"/>
<pin name="AD1" direction="pas"/>
<pin name="AD2" direction="pas"/>
<pin name="AD3" direction="pas"/>
<pin name="AD4" direction="pas"/>
<pin name="AD5" direction="pas"/>
<pin name="AD6" direction="pas"/>
<pin name="AD7" direction="pas"/>
<pin name="AD8" direction="pas"/>
<pin name="AD9" direction="pas"/>
<pin name="AD10" direction="pas"/>
<pin name="AD11" direction="pas"/>
<pin name="AD12" direction="pas"/>
<pin name="AD13" direction="pas"/>
<pin name="AD14" direction="pas"/>
<pin name="AD15" direction="pas"/>
<pin name="AD16" direction="pas"/>
<pin name="AD17" direction="pas"/>
<pin name="AD18" direction="pas"/>
<pin name="AD19" direction="pas"/>
<pin name="AD20" direction="pas"/>
<pin name="AD21" direction="pas"/>
<pin name="AD22" direction="pas"/>
<pin name="AD23" direction="pas"/>
<pin name="AD24" direction="pas"/>
<pin name="AD25" direction="pas"/>
<pin name="AD26" direction="pas"/>
<pin name="AD27" direction="pas"/>
<pin name="AD28" direction="pas"/>
<pin name="AD29" direction="pas"/>
<pin name="AD30" direction="pas"/>
<pin name="AD31" direction="pas"/>
<pin name="C/BE0" direction="pas"/>
<pin name="C/BE1" direction="pas"/>
<pin name="C/BE2" direction="pas"/>
<pin name="C/BE3" direction="pas"/>
<pin name="CLK" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pas"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@18" direction="pas"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="IDSEL" direction="pas"/>
<pin name="NC0" direction="pas"/>
<pin name="NC5" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="PAR" direction="pas"/>
<pin name="SDONE" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="TMS" direction="pas"/>
</symbol>
<symbol name="PCI2_CON">
<pin name="/ACK64" direction="pas"/>
<pin name="/DEVSEL" direction="pas"/>
<pin name="/FRAME" direction="pas"/>
<pin name="/GNT" direction="pas"/>
<pin name="/INTA" direction="pas"/>
<pin name="/INTB" direction="pas"/>
<pin name="/INTC" direction="pas"/>
<pin name="/INTD" direction="pas"/>
<pin name="/IRDY" direction="pas"/>
<pin name="/LOCK" direction="pas"/>
<pin name="/PERR" direction="pas"/>
<pin name="/PRSNT1" direction="pas"/>
<pin name="/PRSNT2" direction="pas"/>
<pin name="/REQ" direction="pas"/>
<pin name="/REQ64" direction="pas"/>
<pin name="/RST" direction="pas"/>
<pin name="/SBO" direction="pas"/>
<pin name="/SERR" direction="pas"/>
<pin name="/STOP" direction="pas"/>
<pin name="/TRDY" direction="pas"/>
<pin name="/TRST" direction="pas"/>
<pin name="+12V" direction="pwr"/>
<pin name="-12V" direction="pwr"/>
<pin name="AD0" direction="pas"/>
<pin name="AD1" direction="pas"/>
<pin name="AD2" direction="pas"/>
<pin name="AD3" direction="pas"/>
<pin name="AD4" direction="pas"/>
<pin name="AD5" direction="pas"/>
<pin name="AD6" direction="pas"/>
<pin name="AD7" direction="pas"/>
<pin name="AD8" direction="pas"/>
<pin name="AD9" direction="pas"/>
<pin name="AD10" direction="pas"/>
<pin name="AD11" direction="pas"/>
<pin name="AD12" direction="pas"/>
<pin name="AD13" direction="pas"/>
<pin name="AD14" direction="pas"/>
<pin name="AD15" direction="pas"/>
<pin name="AD16" direction="pas"/>
<pin name="AD17" direction="pas"/>
<pin name="AD18" direction="pas"/>
<pin name="AD19" direction="pas"/>
<pin name="AD20" direction="pas"/>
<pin name="AD21" direction="pas"/>
<pin name="AD22" direction="pas"/>
<pin name="AD23" direction="pas"/>
<pin name="AD24" direction="pas"/>
<pin name="AD25" direction="pas"/>
<pin name="AD26" direction="pas"/>
<pin name="AD27" direction="pas"/>
<pin name="AD28" direction="pas"/>
<pin name="AD29" direction="pas"/>
<pin name="AD30" direction="pas"/>
<pin name="AD31" direction="pas"/>
<pin name="C/BE0" direction="pas"/>
<pin name="C/BE1" direction="pas"/>
<pin name="C/BE2" direction="pas"/>
<pin name="C/BE3" direction="pas"/>
<pin name="CLK" direction="pas"/>
<pin name="IDSEL" direction="pas"/>
<pin name="PAR" direction="pas"/>
<pin name="SDONE" direction="pas"/>
<pin name="TCK" direction="pas"/>
<pin name="TDI" direction="pas"/>
<pin name="TDO" direction="pas"/>
<pin name="TMS" direction="pas"/>
</symbol>
<symbol name="PCI_PWR">
<pin name="+3,3V" direction="pwr"/>
<pin name="+3,3V@1" direction="pwr"/>
<pin name="+3,3V@2" direction="pwr"/>
<pin name="+3,3V@3" direction="pas"/>
<pin name="+3,3V@4" direction="pwr"/>
<pin name="+3,3V@5" direction="pwr"/>
<pin name="+3,3V@11" direction="pwr"/>
<pin name="+3,3V@10" direction="pwr"/>
<pin name="+3,3V@9" direction="pwr"/>
<pin name="+3,3V@8" direction="pwr"/>
<pin name="+3,3V@7" direction="pwr"/>
<pin name="+3,3V@6" direction="pwr"/>
<pin name="+5V" direction="pwr"/>
<pin name="+5V@1" direction="pwr"/>
<pin name="+5V@2" direction="pwr"/>
<pin name="+5V@3" direction="pwr"/>
<pin name="+5V@4" direction="pwr"/>
<pin name="+5V@5" direction="pwr"/>
<pin name="+5V@6" direction="pwr"/>
<pin name="+5V@12" direction="pwr"/>
<pin name="+5V@11" direction="pwr"/>
<pin name="+5V@10" direction="pwr"/>
<pin name="+5V@9" direction="pwr"/>
<pin name="+5V@8" direction="pwr"/>
<pin name="+5V@7" direction="pwr"/>
<pin name="GND" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="GND@20" direction="pwr"/>
<pin name="GND@21" direction="pas"/>
<pin name="GND@5" direction="pwr"/>
<pin name="GND@6" direction="pwr"/>
<pin name="GND@7" direction="pwr"/>
<pin name="GND@19" direction="pwr"/>
<pin name="GND@18" direction="pwr"/>
<pin name="GND@17" direction="pwr"/>
<pin name="GND@16" direction="pwr"/>
<pin name="GND@15" direction="pwr"/>
<pin name="GND@14" direction="pwr"/>
<pin name="GND@13" direction="pwr"/>
<pin name="GND@12" direction="pwr"/>
<pin name="GND@11" direction="pwr"/>
<pin name="GND@10" direction="pwr"/>
<pin name="GND@9" direction="pwr"/>
<pin name="GND@8" direction="pwr"/>
<pin name="NC0" direction="nc"/>
<pin name="NC5" direction="nc"/>
<pin name="NC1" direction="nc"/>
<pin name="NC2" direction="nc"/>
<pin name="NC3" direction="nc"/>
<pin name="NC4" direction="nc"/>
</symbol>
<symbol name="IBM-AB">
<pin name="SA0"/>
<pin name="SA1"/>
<pin name="SA2"/>
<pin name="SA3"/>
<pin name="SA4"/>
<pin name="SA5"/>
<pin name="SA6"/>
<pin name="SA7"/>
<pin name="SA8"/>
<pin name="SA9"/>
<pin name="SA10"/>
<pin name="SA11"/>
<pin name="SA12"/>
<pin name="SA13"/>
<pin name="SA14"/>
<pin name="SA15"/>
<pin name="SA16"/>
<pin name="SA17"/>
<pin name="SA18"/>
<pin name="SA19"/>
<pin name="AEN" direction="out"/>
<pin name="!IOCHRD" direction="in"/>
<pin name="SD0"/>
<pin name="SD1"/>
<pin name="SD2"/>
<pin name="SD3"/>
<pin name="SD4"/>
<pin name="SD5"/>
<pin name="SD6"/>
<pin name="SD7"/>
<pin name="I/!OCHCK" direction="in"/>
<pin name="GND@0" direction="pwr"/>
<pin name="OSC" direction="out"/>
<pin name="+5V@0" direction="pwr"/>
<pin name="BALE" direction="out"/>
<pin name="T/C" direction="out"/>
<pin name="!DACK2" direction="out"/>
<pin name="IRQ3" direction="in"/>
<pin name="IRQ4" direction="in"/>
<pin name="IRQ5" direction="in"/>
<pin name="IRQ6" direction="in"/>
<pin name="IRQ7" direction="in"/>
<pin name="CLK" direction="out"/>
<pin name="!REFRESH"/>
<pin name="DRQ1" direction="in"/>
<pin name="!DACK1" direction="out"/>
<pin name="DRQ3" direction="in"/>
<pin name="!DACK3" direction="out"/>
<pin name="!IOR"/>
<pin name="!IOW"/>
<pin name="!SMEMR" direction="out"/>
<pin name="!SMEMW" direction="out"/>
<pin name="GND@1" direction="pwr"/>
<pin name="+12V" direction="pwr"/>
<pin name="OWS" direction="in"/>
<pin name="-12V" direction="pwr"/>
<pin name="DRQ2" direction="in"/>
<pin name="-5V" direction="pwr"/>
<pin name="IRQ9" direction="in"/>
<pin name="+5V@1" direction="pwr"/>
<pin name="RESET_DR" direction="out"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="PINQ">
<pin name="1" direction="pas"/>
</symbol>
<symbol name="PIN">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="FEMREC">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="MALE">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="ATPIN">
<pin name="P"/>
</symbol>
<symbol name="FEM">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="FEMRVAL">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="+5V">
<pin name="+5V" direction="pwr"/>
</symbol>
<symbol name="-12V">
<pin name="-12V" direction="pwr"/>
</symbol>
<symbol name="+12V">
<pin name="+12V" direction="pwr"/>
</symbol>
<symbol name="RESERV">
<pin name="RSV" direction="pas"/>
</symbol>
<symbol name="-5V">
<pin name="-5V" direction="pwr"/>
</symbol>
<symbol name="MALEVAL">
<pin name="P" direction="pas"/>
</symbol>
<symbol name="PCI-E-164">
<pin name="A1" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="A3" direction="pas"/>
<pin name="A4" direction="pas"/>
<pin name="A5" direction="pas"/>
<pin name="A6" direction="pas"/>
<pin name="A7" direction="pas"/>
<pin name="A8" direction="pas"/>
<pin name="A9" direction="pas"/>
<pin name="A10" direction="pas"/>
<pin name="A11" direction="pas"/>
<pin name="A12" direction="pas"/>
<pin name="A13" direction="pas"/>
<pin name="A14" direction="pas"/>
<pin name="A15" direction="pas"/>
<pin name="A16" direction="pas"/>
<pin name="A17" direction="pas"/>
<pin name="A18" direction="pas"/>
<pin name="A19" direction="pas"/>
<pin name="A20" direction="pas"/>
<pin name="A21" direction="pas"/>
<pin name="A22" direction="pas"/>
<pin name="A23" direction="pas"/>
<pin name="A24" direction="pas"/>
<pin name="A25" direction="pas"/>
<pin name="A26" direction="pas"/>
<pin name="A27" direction="pas"/>
<pin name="A28" direction="pas"/>
<pin name="A29" direction="pas"/>
<pin name="A30" direction="pas"/>
<pin name="A31" direction="pas"/>
<pin name="A32" direction="pas"/>
<pin name="A33" direction="pas"/>
<pin name="A34" direction="pas"/>
<pin name="A35" direction="pas"/>
<pin name="A36" direction="pas"/>
<pin name="A37" direction="pas"/>
<pin name="A38" direction="pas"/>
<pin name="A39" direction="pas"/>
<pin name="A40" direction="pas"/>
<pin name="A41" direction="pas"/>
<pin name="A42" direction="pas"/>
<pin name="A43" direction="pas"/>
<pin name="A44" direction="pas"/>
<pin name="A45" direction="pas"/>
<pin name="A46" direction="pas"/>
<pin name="A47" direction="pas"/>
<pin name="A48" direction="pas"/>
<pin name="A49" direction="pas"/>
<pin name="A50" direction="pas"/>
<pin name="A51" direction="pas"/>
<pin name="A52" direction="pas"/>
<pin name="A53" direction="pas"/>
<pin name="A54" direction="pas"/>
<pin name="A55" direction="pas"/>
<pin name="A56" direction="pas"/>
<pin name="A57" direction="pas"/>
<pin name="A58" direction="pas"/>
<pin name="A59" direction="pas"/>
<pin name="A60" direction="pas"/>
<pin name="A61" direction="pas"/>
<pin name="A62" direction="pas"/>
<pin name="A63" direction="pas"/>
<pin name="A64" direction="pas"/>
<pin name="A65" direction="pas"/>
<pin name="A66" direction="pas"/>
<pin name="A67" direction="pas"/>
<pin name="A68" direction="pas"/>
<pin name="A69" direction="pas"/>
<pin name="A70" direction="pas"/>
<pin name="A71" direction="pas"/>
<pin name="A72" direction="pas"/>
<pin name="A73" direction="pas"/>
<pin name="A74" direction="pas"/>
<pin name="A75" direction="pas"/>
<pin name="A76" direction="pas"/>
<pin name="A77" direction="pas"/>
<pin name="A78" direction="pas"/>
<pin name="A79" direction="pas"/>
<pin name="A80" direction="pas"/>
<pin name="A81" direction="pas"/>
<pin name="A82" direction="pas"/>
<pin name="B1" direction="pas"/>
<pin name="B2" direction="pas"/>
<pin name="B3" direction="pas"/>
<pin name="B4" direction="pas"/>
<pin name="B5" direction="pas"/>
<pin name="B6" direction="pas"/>
<pin name="B7" direction="pas"/>
<pin name="B8" direction="pas"/>
<pin name="B9" direction="pas"/>
<pin name="B10" direction="pas"/>
<pin name="B11" direction="pas"/>
<pin name="B12" direction="pas"/>
<pin name="B13" direction="pas"/>
<pin name="B14" direction="pas"/>
<pin name="B15" direction="pas"/>
<pin name="B16" direction="pas"/>
<pin name="B17" direction="pas"/>
<pin name="B18" direction="pas"/>
<pin name="B19" direction="pas"/>
<pin name="B20" direction="pas"/>
<pin name="B21" direction="pas"/>
<pin name="B22" direction="pas"/>
<pin name="B23" direction="pas"/>
<pin name="B24" direction="pas"/>
<pin name="B25" direction="pas"/>
<pin name="B26" direction="pas"/>
<pin name="B27" direction="pas"/>
<pin name="B28" direction="pas"/>
<pin name="B29" direction="pas"/>
<pin name="B30" direction="pas"/>
<pin name="B31" direction="pas"/>
<pin name="B32" direction="pas"/>
<pin name="B33" direction="pas"/>
<pin name="B34" direction="pas"/>
<pin name="B35" direction="pas"/>
<pin name="B36" direction="pas"/>
<pin name="B37" direction="pas"/>
<pin name="B38" direction="pas"/>
<pin name="B39" direction="pas"/>
<pin name="B40" direction="pas"/>
<pin name="B41" direction="pas"/>
<pin name="B42" direction="pas"/>
<pin name="B43" direction="pas"/>
<pin name="B44" direction="pas"/>
<pin name="B45" direction="pas"/>
<pin name="B46" direction="pas"/>
<pin name="B47" direction="pas"/>
<pin name="B48" direction="pas"/>
<pin name="B49" direction="pas"/>
<pin name="B50" direction="pas"/>
<pin name="B51" direction="pas"/>
<pin name="B52" direction="pas"/>
<pin name="B53" direction="pas"/>
<pin name="B54" direction="pas"/>
<pin name="B55" direction="pas"/>
<pin name="B56" direction="pas"/>
<pin name="B57" direction="pas"/>
<pin name="B58" direction="pas"/>
<pin name="B59" direction="pas"/>
<pin name="B60" direction="pas"/>
<pin name="B61" direction="pas"/>
<pin name="B62" direction="pas"/>
<pin name="B63" direction="pas"/>
<pin name="B64" direction="pas"/>
<pin name="B65" direction="pas"/>
<pin name="B66" direction="pas"/>
<pin name="B67" direction="pas"/>
<pin name="B68" direction="pas"/>
<pin name="B69" direction="pas"/>
<pin name="B70" direction="pas"/>
<pin name="B71" direction="pas"/>
<pin name="B72" direction="pas"/>
<pin name="B73" direction="pas"/>
<pin name="B74" direction="pas"/>
<pin name="B75" direction="pas"/>
<pin name="B76" direction="pas"/>
<pin name="B77" direction="pas"/>
<pin name="B78" direction="pas"/>
<pin name="B79" direction="pas"/>
<pin name="B80" direction="pas"/>
<pin name="B81" direction="pas"/>
<pin name="B82" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PCI_CON" prefix="CON" uservalue="yes">
<description>&lt;b&gt;PCI BOARD LONG&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCI_CON"/>
</gates>
<devices>
<device name="" package="PCI_BRDL">
<connects>
<connect gate="G$1" pin="+12V" pad="S2"/>
<connect gate="G$1" pin="+3,3V" pad="S21"/>
<connect gate="G$1" pin="+3,3V@1" pad="S27"/>
<connect gate="G$1" pin="+3,3V@10" pad="C31"/>
<connect gate="G$1" pin="+3,3V@11" pad="C25"/>
<connect gate="G$1" pin="+3,3V@2" pad="S33"/>
<connect gate="G$1" pin="+3,3V@3" pad="S39"/>
<connect gate="G$1" pin="+3,3V@4" pad="S45"/>
<connect gate="G$1" pin="+3,3V@5" pad="S53"/>
<connect gate="G$1" pin="+3,3V@6" pad="C54"/>
<connect gate="G$1" pin="+3,3V@7" pad="C43"/>
<connect gate="G$1" pin="+3,3V@8" pad="C41"/>
<connect gate="G$1" pin="+3,3V@9" pad="C36"/>
<connect gate="G$1" pin="+5V" pad="S5"/>
<connect gate="G$1" pin="+5V@1" pad="S8"/>
<connect gate="G$1" pin="+5V@10" pad="C19"/>
<connect gate="G$1" pin="+5V@11" pad="C6"/>
<connect gate="G$1" pin="+5V@12" pad="C5"/>
<connect gate="G$1" pin="+5V@2" pad="S10"/>
<connect gate="G$1" pin="+5V@3" pad="S16"/>
<connect gate="G$1" pin="+5V@4" pad="S59"/>
<connect gate="G$1" pin="+5V@5" pad="S61"/>
<connect gate="G$1" pin="+5V@6" pad="S62"/>
<connect gate="G$1" pin="+5V@7" pad="C62"/>
<connect gate="G$1" pin="+5V@8" pad="C61"/>
<connect gate="G$1" pin="+5V@9" pad="C59"/>
<connect gate="G$1" pin="-12V" pad="C1"/>
<connect gate="G$1" pin="/ACK64" pad="C60"/>
<connect gate="G$1" pin="/DEVSEL" pad="C37"/>
<connect gate="G$1" pin="/FRAME" pad="S34"/>
<connect gate="G$1" pin="/GNT" pad="S17"/>
<connect gate="G$1" pin="/INTA" pad="S6"/>
<connect gate="G$1" pin="/INTB" pad="C7"/>
<connect gate="G$1" pin="/INTC" pad="S7"/>
<connect gate="G$1" pin="/INTD" pad="C8"/>
<connect gate="G$1" pin="/IRDY" pad="C35"/>
<connect gate="G$1" pin="/LOCK" pad="C39"/>
<connect gate="G$1" pin="/PERR" pad="C40"/>
<connect gate="G$1" pin="/PRSNT1" pad="C9"/>
<connect gate="G$1" pin="/PRSNT2" pad="C11"/>
<connect gate="G$1" pin="/REQ" pad="C18"/>
<connect gate="G$1" pin="/REQ64" pad="S60"/>
<connect gate="G$1" pin="/RST" pad="S15"/>
<connect gate="G$1" pin="/SBO" pad="S41"/>
<connect gate="G$1" pin="/SERR" pad="C42"/>
<connect gate="G$1" pin="/STOP" pad="S38"/>
<connect gate="G$1" pin="/TRDY" pad="S36"/>
<connect gate="G$1" pin="/TRST" pad="S1"/>
<connect gate="G$1" pin="AD0" pad="S58"/>
<connect gate="G$1" pin="AD1" pad="C58"/>
<connect gate="G$1" pin="AD10" pad="C48"/>
<connect gate="G$1" pin="AD11" pad="S47"/>
<connect gate="G$1" pin="AD12" pad="C47"/>
<connect gate="G$1" pin="AD13" pad="S46"/>
<connect gate="G$1" pin="AD14" pad="C45"/>
<connect gate="G$1" pin="AD15" pad="S44"/>
<connect gate="G$1" pin="AD16" pad="S32"/>
<connect gate="G$1" pin="AD17" pad="C32"/>
<connect gate="G$1" pin="AD18" pad="S31"/>
<connect gate="G$1" pin="AD19" pad="C30"/>
<connect gate="G$1" pin="AD2" pad="S57"/>
<connect gate="G$1" pin="AD20" pad="S29"/>
<connect gate="G$1" pin="AD21" pad="C29"/>
<connect gate="G$1" pin="AD22" pad="S28"/>
<connect gate="G$1" pin="AD23" pad="C27"/>
<connect gate="G$1" pin="AD24" pad="S25"/>
<connect gate="G$1" pin="AD25" pad="C24"/>
<connect gate="G$1" pin="AD26" pad="S23"/>
<connect gate="G$1" pin="AD27" pad="C23"/>
<connect gate="G$1" pin="AD28" pad="S22"/>
<connect gate="G$1" pin="AD29" pad="C21"/>
<connect gate="G$1" pin="AD3" pad="C56"/>
<connect gate="G$1" pin="AD30" pad="S20"/>
<connect gate="G$1" pin="AD31" pad="C20"/>
<connect gate="G$1" pin="AD4" pad="S55"/>
<connect gate="G$1" pin="AD5" pad="C55"/>
<connect gate="G$1" pin="AD6" pad="S54"/>
<connect gate="G$1" pin="AD7" pad="C53"/>
<connect gate="G$1" pin="AD8" pad="C52"/>
<connect gate="G$1" pin="AD9" pad="S49"/>
<connect gate="G$1" pin="C/BE0" pad="S52"/>
<connect gate="G$1" pin="C/BE1" pad="C44"/>
<connect gate="G$1" pin="C/BE2" pad="C33"/>
<connect gate="G$1" pin="C/BE3" pad="C26"/>
<connect gate="G$1" pin="CLK" pad="C16"/>
<connect gate="G$1" pin="GND" pad="S12"/>
<connect gate="G$1" pin="GND@1" pad="S13"/>
<connect gate="G$1" pin="GND@10" pad="C46"/>
<connect gate="G$1" pin="GND@11" pad="C38"/>
<connect gate="G$1" pin="GND@12" pad="C34"/>
<connect gate="G$1" pin="GND@13" pad="C28"/>
<connect gate="G$1" pin="GND@14" pad="C22"/>
<connect gate="G$1" pin="GND@15" pad="C17"/>
<connect gate="G$1" pin="GND@16" pad="C15"/>
<connect gate="G$1" pin="GND@17" pad="C13"/>
<connect gate="G$1" pin="GND@18" pad="C12"/>
<connect gate="G$1" pin="GND@19" pad="C3"/>
<connect gate="G$1" pin="GND@2" pad="S18"/>
<connect gate="G$1" pin="GND@20" pad="S35"/>
<connect gate="G$1" pin="GND@21" pad="S37"/>
<connect gate="G$1" pin="GND@3" pad="S24"/>
<connect gate="G$1" pin="GND@4" pad="S30"/>
<connect gate="G$1" pin="GND@5" pad="S42"/>
<connect gate="G$1" pin="GND@6" pad="S48"/>
<connect gate="G$1" pin="GND@7" pad="S56"/>
<connect gate="G$1" pin="GND@8" pad="C57"/>
<connect gate="G$1" pin="GND@9" pad="C49"/>
<connect gate="G$1" pin="IDSEL" pad="S26"/>
<connect gate="G$1" pin="NC0" pad="S9"/>
<connect gate="G$1" pin="NC1" pad="S14"/>
<connect gate="G$1" pin="NC2" pad="S19"/>
<connect gate="G$1" pin="NC3" pad="C10"/>
<connect gate="G$1" pin="NC4" pad="C14"/>
<connect gate="G$1" pin="NC5" pad="S11"/>
<connect gate="G$1" pin="PAR" pad="S43"/>
<connect gate="G$1" pin="SDONE" pad="S40"/>
<connect gate="G$1" pin="TCK" pad="C2"/>
<connect gate="G$1" pin="TDI" pad="S4"/>
<connect gate="G$1" pin="TDO" pad="C4"/>
<connect gate="G$1" pin="TMS" pad="S3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCI2-SLOT" prefix="ST" uservalue="yes">
<description>&lt;b&gt;PCI BOARD SHORT&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PCI2_CON"/>
<gate name="P" symbol="PCI_PWR"/>
</gates>
<devices>
<device name="" package="PCI_BRD">
<connects>
<connect gate="G$1" pin="+12V" pad="S2"/>
<connect gate="G$1" pin="-12V" pad="C1"/>
<connect gate="G$1" pin="/ACK64" pad="C60"/>
<connect gate="G$1" pin="/DEVSEL" pad="C37"/>
<connect gate="G$1" pin="/FRAME" pad="S34"/>
<connect gate="G$1" pin="/GNT" pad="S17"/>
<connect gate="G$1" pin="/INTA" pad="S6"/>
<connect gate="G$1" pin="/INTB" pad="C7"/>
<connect gate="G$1" pin="/INTC" pad="S7"/>
<connect gate="G$1" pin="/INTD" pad="C8"/>
<connect gate="G$1" pin="/IRDY" pad="C35"/>
<connect gate="G$1" pin="/LOCK" pad="C39"/>
<connect gate="G$1" pin="/PERR" pad="C40"/>
<connect gate="G$1" pin="/PRSNT1" pad="C9"/>
<connect gate="G$1" pin="/PRSNT2" pad="C11"/>
<connect gate="G$1" pin="/REQ" pad="C18"/>
<connect gate="G$1" pin="/REQ64" pad="S60"/>
<connect gate="G$1" pin="/RST" pad="S15"/>
<connect gate="G$1" pin="/SBO" pad="S41"/>
<connect gate="G$1" pin="/SERR" pad="C42"/>
<connect gate="G$1" pin="/STOP" pad="S38"/>
<connect gate="G$1" pin="/TRDY" pad="S36"/>
<connect gate="G$1" pin="/TRST" pad="S1"/>
<connect gate="G$1" pin="AD0" pad="S58"/>
<connect gate="G$1" pin="AD1" pad="C58"/>
<connect gate="G$1" pin="AD10" pad="C48"/>
<connect gate="G$1" pin="AD11" pad="S47"/>
<connect gate="G$1" pin="AD12" pad="C47"/>
<connect gate="G$1" pin="AD13" pad="S46"/>
<connect gate="G$1" pin="AD14" pad="C45"/>
<connect gate="G$1" pin="AD15" pad="S44"/>
<connect gate="G$1" pin="AD16" pad="S32"/>
<connect gate="G$1" pin="AD17" pad="C32"/>
<connect gate="G$1" pin="AD18" pad="S31"/>
<connect gate="G$1" pin="AD19" pad="C30"/>
<connect gate="G$1" pin="AD2" pad="S57"/>
<connect gate="G$1" pin="AD20" pad="S29"/>
<connect gate="G$1" pin="AD21" pad="C29"/>
<connect gate="G$1" pin="AD22" pad="S28"/>
<connect gate="G$1" pin="AD23" pad="C27"/>
<connect gate="G$1" pin="AD24" pad="S25"/>
<connect gate="G$1" pin="AD25" pad="C24"/>
<connect gate="G$1" pin="AD26" pad="S23"/>
<connect gate="G$1" pin="AD27" pad="C23"/>
<connect gate="G$1" pin="AD28" pad="S22"/>
<connect gate="G$1" pin="AD29" pad="C21"/>
<connect gate="G$1" pin="AD3" pad="C56"/>
<connect gate="G$1" pin="AD30" pad="S20"/>
<connect gate="G$1" pin="AD31" pad="C20"/>
<connect gate="G$1" pin="AD4" pad="S55"/>
<connect gate="G$1" pin="AD5" pad="C55"/>
<connect gate="G$1" pin="AD6" pad="S54"/>
<connect gate="G$1" pin="AD7" pad="C53"/>
<connect gate="G$1" pin="AD8" pad="C52"/>
<connect gate="G$1" pin="AD9" pad="S49"/>
<connect gate="G$1" pin="C/BE0" pad="S52"/>
<connect gate="G$1" pin="C/BE1" pad="C44"/>
<connect gate="G$1" pin="C/BE2" pad="C33"/>
<connect gate="G$1" pin="C/BE3" pad="C26"/>
<connect gate="G$1" pin="CLK" pad="C16"/>
<connect gate="G$1" pin="IDSEL" pad="S26"/>
<connect gate="G$1" pin="PAR" pad="S43"/>
<connect gate="G$1" pin="SDONE" pad="S40"/>
<connect gate="G$1" pin="TCK" pad="C2"/>
<connect gate="G$1" pin="TDI" pad="S4"/>
<connect gate="G$1" pin="TDO" pad="C4"/>
<connect gate="G$1" pin="TMS" pad="S3"/>
<connect gate="P" pin="+3,3V" pad="S21"/>
<connect gate="P" pin="+3,3V@1" pad="S27"/>
<connect gate="P" pin="+3,3V@10" pad="C31"/>
<connect gate="P" pin="+3,3V@11" pad="C25"/>
<connect gate="P" pin="+3,3V@2" pad="S33"/>
<connect gate="P" pin="+3,3V@3" pad="S39"/>
<connect gate="P" pin="+3,3V@4" pad="S45"/>
<connect gate="P" pin="+3,3V@5" pad="S53"/>
<connect gate="P" pin="+3,3V@6" pad="C54"/>
<connect gate="P" pin="+3,3V@7" pad="C43"/>
<connect gate="P" pin="+3,3V@8" pad="C41"/>
<connect gate="P" pin="+3,3V@9" pad="C36"/>
<connect gate="P" pin="+5V" pad="S5"/>
<connect gate="P" pin="+5V@1" pad="S8"/>
<connect gate="P" pin="+5V@10" pad="C19"/>
<connect gate="P" pin="+5V@11" pad="C6"/>
<connect gate="P" pin="+5V@12" pad="C5"/>
<connect gate="P" pin="+5V@2" pad="S10"/>
<connect gate="P" pin="+5V@3" pad="S16"/>
<connect gate="P" pin="+5V@4" pad="S59"/>
<connect gate="P" pin="+5V@5" pad="S61"/>
<connect gate="P" pin="+5V@6" pad="S62"/>
<connect gate="P" pin="+5V@7" pad="C62"/>
<connect gate="P" pin="+5V@8" pad="C61"/>
<connect gate="P" pin="+5V@9" pad="C59"/>
<connect gate="P" pin="GND" pad="S12"/>
<connect gate="P" pin="GND@1" pad="S13"/>
<connect gate="P" pin="GND@10" pad="C46"/>
<connect gate="P" pin="GND@11" pad="C38"/>
<connect gate="P" pin="GND@12" pad="C34"/>
<connect gate="P" pin="GND@13" pad="C28"/>
<connect gate="P" pin="GND@14" pad="C22"/>
<connect gate="P" pin="GND@15" pad="C17"/>
<connect gate="P" pin="GND@16" pad="C15"/>
<connect gate="P" pin="GND@17" pad="C13"/>
<connect gate="P" pin="GND@18" pad="C12"/>
<connect gate="P" pin="GND@19" pad="C3"/>
<connect gate="P" pin="GND@2" pad="S18"/>
<connect gate="P" pin="GND@20" pad="S37"/>
<connect gate="P" pin="GND@21" pad="S35"/>
<connect gate="P" pin="GND@3" pad="S24"/>
<connect gate="P" pin="GND@4" pad="S30"/>
<connect gate="P" pin="GND@5" pad="S42"/>
<connect gate="P" pin="GND@6" pad="S48"/>
<connect gate="P" pin="GND@7" pad="S56"/>
<connect gate="P" pin="GND@8" pad="C57"/>
<connect gate="P" pin="GND@9" pad="C49"/>
<connect gate="P" pin="NC0" pad="S9"/>
<connect gate="P" pin="NC1" pad="S14"/>
<connect gate="P" pin="NC2" pad="S19"/>
<connect gate="P" pin="NC3" pad="C10"/>
<connect gate="P" pin="NC4" pad="C14"/>
<connect gate="P" pin="NC5" pad="S11"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IBMAB" prefix="ST" uservalue="yes">
<description>&lt;B&gt;8-bit CARD IBM/PC-AT&lt;/B&gt;</description>
<gates>
<gate name="G$1" symbol="IBM-AB"/>
</gates>
<devices>
<device name="" package="IBM_8AB">
<connects>
<connect gate="G$1" pin="!DACK1" pad="B17"/>
<connect gate="G$1" pin="!DACK2" pad="B26"/>
<connect gate="G$1" pin="!DACK3" pad="B15"/>
<connect gate="G$1" pin="!IOCHRD" pad="A10"/>
<connect gate="G$1" pin="!IOR" pad="B14"/>
<connect gate="G$1" pin="!IOW" pad="B13"/>
<connect gate="G$1" pin="!REFRESH" pad="B19"/>
<connect gate="G$1" pin="!SMEMR" pad="B12"/>
<connect gate="G$1" pin="!SMEMW" pad="B11"/>
<connect gate="G$1" pin="+12V" pad="B9"/>
<connect gate="G$1" pin="+5V@0" pad="B29"/>
<connect gate="G$1" pin="+5V@1" pad="B3"/>
<connect gate="G$1" pin="-12V" pad="B7"/>
<connect gate="G$1" pin="-5V" pad="B5"/>
<connect gate="G$1" pin="AEN" pad="A11"/>
<connect gate="G$1" pin="BALE" pad="B28"/>
<connect gate="G$1" pin="CLK" pad="B20"/>
<connect gate="G$1" pin="DRQ1" pad="B18"/>
<connect gate="G$1" pin="DRQ2" pad="B6"/>
<connect gate="G$1" pin="DRQ3" pad="B16"/>
<connect gate="G$1" pin="GND@0" pad="B31"/>
<connect gate="G$1" pin="GND@1" pad="B10"/>
<connect gate="G$1" pin="GND@2" pad="B1"/>
<connect gate="G$1" pin="I/!OCHCK" pad="A1"/>
<connect gate="G$1" pin="IRQ3" pad="B25"/>
<connect gate="G$1" pin="IRQ4" pad="B24"/>
<connect gate="G$1" pin="IRQ5" pad="B23"/>
<connect gate="G$1" pin="IRQ6" pad="B22"/>
<connect gate="G$1" pin="IRQ7" pad="B21"/>
<connect gate="G$1" pin="IRQ9" pad="B4"/>
<connect gate="G$1" pin="OSC" pad="B30"/>
<connect gate="G$1" pin="OWS" pad="B8"/>
<connect gate="G$1" pin="RESET_DR" pad="B2"/>
<connect gate="G$1" pin="SA0" pad="A31"/>
<connect gate="G$1" pin="SA1" pad="A30"/>
<connect gate="G$1" pin="SA10" pad="A21"/>
<connect gate="G$1" pin="SA11" pad="A20"/>
<connect gate="G$1" pin="SA12" pad="A19"/>
<connect gate="G$1" pin="SA13" pad="A18"/>
<connect gate="G$1" pin="SA14" pad="A17"/>
<connect gate="G$1" pin="SA15" pad="A16"/>
<connect gate="G$1" pin="SA16" pad="A15"/>
<connect gate="G$1" pin="SA17" pad="A14"/>
<connect gate="G$1" pin="SA18" pad="A13"/>
<connect gate="G$1" pin="SA19" pad="A12"/>
<connect gate="G$1" pin="SA2" pad="A29"/>
<connect gate="G$1" pin="SA3" pad="A28"/>
<connect gate="G$1" pin="SA4" pad="A27"/>
<connect gate="G$1" pin="SA5" pad="A26"/>
<connect gate="G$1" pin="SA6" pad="A25"/>
<connect gate="G$1" pin="SA7" pad="A24"/>
<connect gate="G$1" pin="SA8" pad="A23"/>
<connect gate="G$1" pin="SA9" pad="A22"/>
<connect gate="G$1" pin="SD0" pad="A9"/>
<connect gate="G$1" pin="SD1" pad="A8"/>
<connect gate="G$1" pin="SD2" pad="A7"/>
<connect gate="G$1" pin="SD3" pad="A6"/>
<connect gate="G$1" pin="SD4" pad="A5"/>
<connect gate="G$1" pin="SD5" pad="A4"/>
<connect gate="G$1" pin="SD6" pad="A3"/>
<connect gate="G$1" pin="SD7" pad="A2"/>
<connect gate="G$1" pin="T/C" pad="B27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IBM16BIT" prefix="ST" uservalue="yes">
<description>&lt;B&gt;16-bit CARD IBM/PC-AT&lt;/B&gt;</description>
<gates>
<gate name="_I/OCHK\" symbol="ATPIN"/>
<gate name="_D7" symbol="ATPIN"/>
<gate name="_D6" symbol="ATPIN"/>
<gate name="_D5" symbol="ATPIN"/>
<gate name="_D4" symbol="ATPIN"/>
<gate name="_D3" symbol="ATPIN"/>
<gate name="_D2" symbol="ATPIN"/>
<gate name="_D1" symbol="ATPIN"/>
<gate name="_D0" symbol="ATPIN"/>
<gate name="_I/ORDY" symbol="ATPIN"/>
<gate name="_AEN" symbol="ATPIN"/>
<gate name="_A19" symbol="ATPIN"/>
<gate name="_A18" symbol="ATPIN"/>
<gate name="_A17" symbol="ATPIN"/>
<gate name="_A16" symbol="ATPIN"/>
<gate name="_A15" symbol="ATPIN"/>
<gate name="_A14" symbol="ATPIN"/>
<gate name="_A13" symbol="ATPIN"/>
<gate name="_A12" symbol="ATPIN"/>
<gate name="_A11" symbol="ATPIN"/>
<gate name="_A10" symbol="ATPIN"/>
<gate name="_A9" symbol="ATPIN"/>
<gate name="_A8" symbol="ATPIN"/>
<gate name="_A7" symbol="ATPIN"/>
<gate name="_A6" symbol="ATPIN"/>
<gate name="_A5" symbol="ATPIN"/>
<gate name="_A4" symbol="ATPIN"/>
<gate name="_A3" symbol="ATPIN"/>
<gate name="_A2" symbol="ATPIN"/>
<gate name="_A1" symbol="ATPIN"/>
<gate name="_A0" symbol="ATPIN"/>
<gate name="_GND@3" symbol="ATPIN"/>
<gate name="_RESET" symbol="ATPIN"/>
<gate name="_+5V@2" symbol="ATPIN"/>
<gate name="_IRQ9" symbol="ATPIN"/>
<gate name="_-5V" symbol="ATPIN"/>
<gate name="_DRQ2" symbol="ATPIN"/>
<gate name="_-12V" symbol="ATPIN"/>
<gate name="_CARDS" symbol="ATPIN"/>
<gate name="_+12V" symbol="ATPIN"/>
<gate name="_GND@2" symbol="ATPIN"/>
<gate name="_MEMW\" symbol="ATPIN"/>
<gate name="_MEMR\" symbol="ATPIN"/>
<gate name="_IOW\" symbol="ATPIN"/>
<gate name="_IOR\" symbol="ATPIN"/>
<gate name="_DACK3\" symbol="ATPIN"/>
<gate name="_DRQ3" symbol="ATPIN"/>
<gate name="_DACK1\" symbol="ATPIN"/>
<gate name="_DRQ1" symbol="ATPIN"/>
<gate name="_REFRS" symbol="ATPIN"/>
<gate name="_CLK" symbol="ATPIN"/>
<gate name="_IRQ7" symbol="ATPIN"/>
<gate name="_IRQ6" symbol="ATPIN"/>
<gate name="_IRQ5" symbol="ATPIN"/>
<gate name="_IRQ4" symbol="ATPIN"/>
<gate name="_IRQ3" symbol="ATPIN"/>
<gate name="_DACK2\" symbol="ATPIN"/>
<gate name="_T/C" symbol="ATPIN"/>
<gate name="_ALE" symbol="ATPIN"/>
<gate name="_+5V@1" symbol="ATPIN"/>
<gate name="_OSC" symbol="ATPIN"/>
<gate name="_GND@1" symbol="ATPIN"/>
<gate name="_SBHE" symbol="ATPIN"/>
<gate name="_LA23" symbol="ATPIN"/>
<gate name="_LA22" symbol="ATPIN"/>
<gate name="_LA21" symbol="ATPIN"/>
<gate name="_LA20" symbol="ATPIN"/>
<gate name="_LA19" symbol="ATPIN"/>
<gate name="_LA18" symbol="ATPIN"/>
<gate name="_LA17" symbol="ATPIN"/>
<gate name="_MEM_R" symbol="ATPIN"/>
<gate name="_MEM_W" symbol="ATPIN"/>
<gate name="_D8" symbol="ATPIN"/>
<gate name="_D9" symbol="ATPIN"/>
<gate name="_D10" symbol="ATPIN"/>
<gate name="_D11" symbol="ATPIN"/>
<gate name="_D12" symbol="ATPIN"/>
<gate name="_D13" symbol="ATPIN"/>
<gate name="_D14" symbol="ATPIN"/>
<gate name="_D15" symbol="ATPIN"/>
<gate name="_MEMCS16" symbol="ATPIN"/>
<gate name="_I/OCS16" symbol="ATPIN"/>
<gate name="_IRQ10" symbol="ATPIN"/>
<gate name="_IRQ11" symbol="ATPIN"/>
<gate name="_IRQ12" symbol="ATPIN"/>
<gate name="_IRQ15" symbol="ATPIN"/>
<gate name="_IRQ14" symbol="ATPIN"/>
<gate name="_DACK0" symbol="ATPIN"/>
<gate name="_DRQ0" symbol="ATPIN"/>
<gate name="_DACK5" symbol="ATPIN"/>
<gate name="_DRQ5" symbol="ATPIN"/>
<gate name="_DACK6" symbol="ATPIN"/>
<gate name="_DRQ6" symbol="ATPIN"/>
<gate name="_DACK7" symbol="ATPIN"/>
<gate name="_DRQ7" symbol="ATPIN"/>
<gate name="_+5V@3" symbol="ATPIN"/>
<gate name="_MASTER" symbol="ATPIN"/>
<gate name="_GND@4" symbol="ATPIN"/>
</gates>
<devices>
<device name="" package="IBM16BIT">
<connects>
<connect gate="_+12V" pin="P" pad="B9"/>
<connect gate="_+5V@1" pin="P" pad="B29"/>
<connect gate="_+5V@2" pin="P" pad="B3"/>
<connect gate="_+5V@3" pin="P" pad="D16"/>
<connect gate="_-12V" pin="P" pad="B7"/>
<connect gate="_-5V" pin="P" pad="B5"/>
<connect gate="_A0" pin="P" pad="A31"/>
<connect gate="_A1" pin="P" pad="A30"/>
<connect gate="_A10" pin="P" pad="A21"/>
<connect gate="_A11" pin="P" pad="A20"/>
<connect gate="_A12" pin="P" pad="A19"/>
<connect gate="_A13" pin="P" pad="A18"/>
<connect gate="_A14" pin="P" pad="A17"/>
<connect gate="_A15" pin="P" pad="A16"/>
<connect gate="_A16" pin="P" pad="A15"/>
<connect gate="_A17" pin="P" pad="A14"/>
<connect gate="_A18" pin="P" pad="A13"/>
<connect gate="_A19" pin="P" pad="A12"/>
<connect gate="_A2" pin="P" pad="A29"/>
<connect gate="_A3" pin="P" pad="A28"/>
<connect gate="_A4" pin="P" pad="A27"/>
<connect gate="_A5" pin="P" pad="A26"/>
<connect gate="_A6" pin="P" pad="A25"/>
<connect gate="_A7" pin="P" pad="A24"/>
<connect gate="_A8" pin="P" pad="A23"/>
<connect gate="_A9" pin="P" pad="A22"/>
<connect gate="_AEN" pin="P" pad="A11"/>
<connect gate="_ALE" pin="P" pad="B28"/>
<connect gate="_CARDS" pin="P" pad="B8"/>
<connect gate="_CLK" pin="P" pad="B20"/>
<connect gate="_D0" pin="P" pad="A9"/>
<connect gate="_D1" pin="P" pad="A8"/>
<connect gate="_D10" pin="P" pad="C13"/>
<connect gate="_D11" pin="P" pad="C14"/>
<connect gate="_D12" pin="P" pad="C15"/>
<connect gate="_D13" pin="P" pad="C16"/>
<connect gate="_D14" pin="P" pad="C17"/>
<connect gate="_D15" pin="P" pad="C18"/>
<connect gate="_D2" pin="P" pad="A7"/>
<connect gate="_D3" pin="P" pad="A6"/>
<connect gate="_D4" pin="P" pad="A5"/>
<connect gate="_D5" pin="P" pad="A4"/>
<connect gate="_D6" pin="P" pad="A3"/>
<connect gate="_D7" pin="P" pad="A2"/>
<connect gate="_D8" pin="P" pad="C11"/>
<connect gate="_D9" pin="P" pad="C12"/>
<connect gate="_DACK0" pin="P" pad="D8"/>
<connect gate="_DACK1\" pin="P" pad="B17"/>
<connect gate="_DACK2\" pin="P" pad="B26"/>
<connect gate="_DACK3\" pin="P" pad="B15"/>
<connect gate="_DACK5" pin="P" pad="D10"/>
<connect gate="_DACK6" pin="P" pad="D12"/>
<connect gate="_DACK7" pin="P" pad="D14"/>
<connect gate="_DRQ0" pin="P" pad="D9"/>
<connect gate="_DRQ1" pin="P" pad="B18"/>
<connect gate="_DRQ2" pin="P" pad="B6"/>
<connect gate="_DRQ3" pin="P" pad="B16"/>
<connect gate="_DRQ5" pin="P" pad="D11"/>
<connect gate="_DRQ6" pin="P" pad="D13"/>
<connect gate="_DRQ7" pin="P" pad="D15"/>
<connect gate="_GND@1" pin="P" pad="B31"/>
<connect gate="_GND@2" pin="P" pad="B10"/>
<connect gate="_GND@3" pin="P" pad="B1"/>
<connect gate="_GND@4" pin="P" pad="D18"/>
<connect gate="_I/OCHK\" pin="P" pad="A1"/>
<connect gate="_I/OCS16" pin="P" pad="D2"/>
<connect gate="_I/ORDY" pin="P" pad="A10"/>
<connect gate="_IOR\" pin="P" pad="B14"/>
<connect gate="_IOW\" pin="P" pad="B13"/>
<connect gate="_IRQ10" pin="P" pad="D3"/>
<connect gate="_IRQ11" pin="P" pad="D4"/>
<connect gate="_IRQ12" pin="P" pad="D5"/>
<connect gate="_IRQ14" pin="P" pad="D7"/>
<connect gate="_IRQ15" pin="P" pad="D6"/>
<connect gate="_IRQ3" pin="P" pad="B25"/>
<connect gate="_IRQ4" pin="P" pad="B24"/>
<connect gate="_IRQ5" pin="P" pad="B23"/>
<connect gate="_IRQ6" pin="P" pad="B22"/>
<connect gate="_IRQ7" pin="P" pad="B21"/>
<connect gate="_IRQ9" pin="P" pad="B4"/>
<connect gate="_LA17" pin="P" pad="C8"/>
<connect gate="_LA18" pin="P" pad="C7"/>
<connect gate="_LA19" pin="P" pad="C6"/>
<connect gate="_LA20" pin="P" pad="C5"/>
<connect gate="_LA21" pin="P" pad="C4"/>
<connect gate="_LA22" pin="P" pad="C3"/>
<connect gate="_LA23" pin="P" pad="C2"/>
<connect gate="_MASTER" pin="P" pad="D17"/>
<connect gate="_MEMCS16" pin="P" pad="D1"/>
<connect gate="_MEMR\" pin="P" pad="B12"/>
<connect gate="_MEMW\" pin="P" pad="B11"/>
<connect gate="_MEM_R" pin="P" pad="C9"/>
<connect gate="_MEM_W" pin="P" pad="C10"/>
<connect gate="_OSC" pin="P" pad="B30"/>
<connect gate="_REFRS" pin="P" pad="B19"/>
<connect gate="_RESET" pin="P" pad="B2"/>
<connect gate="_SBHE" pin="P" pad="C1"/>
<connect gate="_T/C" pin="P" pad="B27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IBM8BIT" prefix="ST" uservalue="yes">
<description>&lt;B&gt;8-bit CARD IBM/PC-AT&lt;/B&gt;</description>
<gates>
<gate name="_I/OCHK\" symbol="ATPIN"/>
<gate name="_D7" symbol="ATPIN"/>
<gate name="_D6" symbol="ATPIN"/>
<gate name="_D5" symbol="ATPIN"/>
<gate name="_D4" symbol="ATPIN"/>
<gate name="_D3" symbol="ATPIN"/>
<gate name="_D2" symbol="ATPIN"/>
<gate name="_D1" symbol="ATPIN"/>
<gate name="_D0" symbol="ATPIN"/>
<gate name="_I/ORDY" symbol="ATPIN"/>
<gate name="_AEN" symbol="ATPIN"/>
<gate name="_A19" symbol="ATPIN"/>
<gate name="_A18" symbol="ATPIN"/>
<gate name="_A17" symbol="ATPIN"/>
<gate name="_A16" symbol="ATPIN"/>
<gate name="_A15" symbol="ATPIN"/>
<gate name="_A14" symbol="ATPIN"/>
<gate name="_A13" symbol="ATPIN"/>
<gate name="_A12" symbol="ATPIN"/>
<gate name="_A11" symbol="ATPIN"/>
<gate name="_A10" symbol="ATPIN"/>
<gate name="_A9" symbol="ATPIN"/>
<gate name="_A8" symbol="ATPIN"/>
<gate name="_A7" symbol="ATPIN"/>
<gate name="_A6" symbol="ATPIN"/>
<gate name="_A5" symbol="ATPIN"/>
<gate name="_A4" symbol="ATPIN"/>
<gate name="_A3" symbol="ATPIN"/>
<gate name="_A2" symbol="ATPIN"/>
<gate name="_A1" symbol="ATPIN"/>
<gate name="_A0" symbol="ATPIN"/>
<gate name="_GND@3" symbol="ATPIN"/>
<gate name="_RESET" symbol="ATPIN"/>
<gate name="_+5V@2" symbol="ATPIN"/>
<gate name="_IRQ9" symbol="ATPIN"/>
<gate name="_-5V" symbol="ATPIN"/>
<gate name="_DRQ2" symbol="ATPIN"/>
<gate name="_-12V" symbol="ATPIN"/>
<gate name="_CARDS" symbol="ATPIN"/>
<gate name="_+12V" symbol="ATPIN"/>
<gate name="_GND@2" symbol="ATPIN"/>
<gate name="_MEMW\" symbol="ATPIN"/>
<gate name="_MEMR\" symbol="ATPIN"/>
<gate name="_IOW\" symbol="ATPIN"/>
<gate name="_IOR\" symbol="ATPIN"/>
<gate name="_DACK3\" symbol="ATPIN"/>
<gate name="_DRQ3" symbol="ATPIN"/>
<gate name="_DACK1\" symbol="ATPIN"/>
<gate name="_DRQ1" symbol="ATPIN"/>
<gate name="_REFRS" symbol="ATPIN"/>
<gate name="_CLK" symbol="ATPIN"/>
<gate name="_IRQ7" symbol="ATPIN"/>
<gate name="_IRQ6" symbol="ATPIN"/>
<gate name="_IRQ5" symbol="ATPIN"/>
<gate name="_IRQ4" symbol="ATPIN"/>
<gate name="_IRQ3" symbol="ATPIN"/>
<gate name="_DACK2\" symbol="ATPIN"/>
<gate name="_T/C" symbol="ATPIN"/>
<gate name="_ALE" symbol="ATPIN"/>
<gate name="_+5V@1" symbol="ATPIN"/>
<gate name="_OSC" symbol="ATPIN"/>
<gate name="_GND@1" symbol="ATPIN"/>
</gates>
<devices>
<device name="" package="IBM8BIT">
<connects>
<connect gate="_+12V" pin="P" pad="B9"/>
<connect gate="_+5V@1" pin="P" pad="B29"/>
<connect gate="_+5V@2" pin="P" pad="B3"/>
<connect gate="_-12V" pin="P" pad="B7"/>
<connect gate="_-5V" pin="P" pad="B5"/>
<connect gate="_A0" pin="P" pad="A31"/>
<connect gate="_A1" pin="P" pad="A30"/>
<connect gate="_A10" pin="P" pad="A21"/>
<connect gate="_A11" pin="P" pad="A20"/>
<connect gate="_A12" pin="P" pad="A19"/>
<connect gate="_A13" pin="P" pad="A18"/>
<connect gate="_A14" pin="P" pad="A17"/>
<connect gate="_A15" pin="P" pad="A16"/>
<connect gate="_A16" pin="P" pad="A15"/>
<connect gate="_A17" pin="P" pad="A14"/>
<connect gate="_A18" pin="P" pad="A13"/>
<connect gate="_A19" pin="P" pad="A12"/>
<connect gate="_A2" pin="P" pad="A29"/>
<connect gate="_A3" pin="P" pad="A28"/>
<connect gate="_A4" pin="P" pad="A27"/>
<connect gate="_A5" pin="P" pad="A26"/>
<connect gate="_A6" pin="P" pad="A25"/>
<connect gate="_A7" pin="P" pad="A24"/>
<connect gate="_A8" pin="P" pad="A23"/>
<connect gate="_A9" pin="P" pad="A22"/>
<connect gate="_AEN" pin="P" pad="A11"/>
<connect gate="_ALE" pin="P" pad="B28"/>
<connect gate="_CARDS" pin="P" pad="B8"/>
<connect gate="_CLK" pin="P" pad="B20"/>
<connect gate="_D0" pin="P" pad="A9"/>
<connect gate="_D1" pin="P" pad="A8"/>
<connect gate="_D2" pin="P" pad="A7"/>
<connect gate="_D3" pin="P" pad="A6"/>
<connect gate="_D4" pin="P" pad="A5"/>
<connect gate="_D5" pin="P" pad="A4"/>
<connect gate="_D6" pin="P" pad="A3"/>
<connect gate="_D7" pin="P" pad="A2"/>
<connect gate="_DACK1\" pin="P" pad="B17"/>
<connect gate="_DACK2\" pin="P" pad="B26"/>
<connect gate="_DACK3\" pin="P" pad="B15"/>
<connect gate="_DRQ1" pin="P" pad="B18"/>
<connect gate="_DRQ2" pin="P" pad="B6"/>
<connect gate="_DRQ3" pin="P" pad="B16"/>
<connect gate="_GND@1" pin="P" pad="B31"/>
<connect gate="_GND@2" pin="P" pad="B10"/>
<connect gate="_GND@3" pin="P" pad="B1"/>
<connect gate="_I/OCHK\" pin="P" pad="A1"/>
<connect gate="_I/ORDY" pin="P" pad="A10"/>
<connect gate="_IOR\" pin="P" pad="B14"/>
<connect gate="_IOW\" pin="P" pad="B13"/>
<connect gate="_IRQ3" pin="P" pad="B25"/>
<connect gate="_IRQ4" pin="P" pad="B24"/>
<connect gate="_IRQ5" pin="P" pad="B23"/>
<connect gate="_IRQ6" pin="P" pad="B22"/>
<connect gate="_IRQ7" pin="P" pad="B21"/>
<connect gate="_IRQ9" pin="P" pad="B4"/>
<connect gate="_MEMR\" pin="P" pad="B12"/>
<connect gate="_MEMW\" pin="P" pad="B11"/>
<connect gate="_OSC" pin="P" pad="B30"/>
<connect gate="_REFRS" pin="P" pad="B19"/>
<connect gate="_RESET" pin="P" pad="B2"/>
<connect gate="_T/C" pin="P" pad="B27"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ISA-SLOT" prefix="X" uservalue="yes">
<description>&lt;B&gt;ISA SLOT&lt;/B&gt;</description>
<gates>
<gate name="-A2" symbol="FEMREC"/>
<gate name="-A3" symbol="FEMREC"/>
<gate name="-A4" symbol="FEMREC"/>
<gate name="-A5" symbol="FEMREC"/>
<gate name="-A6" symbol="FEMREC"/>
<gate name="-A7" symbol="FEMREC"/>
<gate name="-A8" symbol="FEMREC"/>
<gate name="-A9" symbol="FEMREC"/>
<gate name="-A10" symbol="FEMREC"/>
<gate name="-A11" symbol="FEMREC"/>
<gate name="-A12" symbol="FEMREC"/>
<gate name="-A13" symbol="FEMREC"/>
<gate name="-A14" symbol="FEMREC"/>
<gate name="-A15" symbol="FEMREC"/>
<gate name="-A16" symbol="FEMREC"/>
<gate name="-A17" symbol="FEMREC"/>
<gate name="-A18" symbol="FEMREC"/>
<gate name="-A19" symbol="FEMREC"/>
<gate name="-A20" symbol="FEMREC"/>
<gate name="-A21" symbol="FEMREC"/>
<gate name="-A22" symbol="FEMREC"/>
<gate name="-A23" symbol="FEMREC"/>
<gate name="-A24" symbol="FEMREC"/>
<gate name="-A25" symbol="FEMREC"/>
<gate name="-A26" symbol="FEMREC"/>
<gate name="-A27" symbol="FEMREC"/>
<gate name="-A28" symbol="FEMREC"/>
<gate name="-A29" symbol="FEMREC"/>
<gate name="-A30" symbol="FEMREC"/>
<gate name="-A31" symbol="FEMREC"/>
<gate name="-B2" symbol="FEMREC"/>
<gate name="-B3" symbol="FEMREC"/>
<gate name="-B4" symbol="FEMREC"/>
<gate name="-B5" symbol="FEMREC"/>
<gate name="-B6" symbol="FEMREC"/>
<gate name="-B7" symbol="FEMREC"/>
<gate name="-B8" symbol="FEMREC"/>
<gate name="-B9" symbol="FEMREC"/>
<gate name="-B10" symbol="FEMREC"/>
<gate name="-B11" symbol="FEMREC"/>
<gate name="-B12" symbol="FEMREC"/>
<gate name="-B13" symbol="FEMREC"/>
<gate name="-B14" symbol="FEMREC"/>
<gate name="-B15" symbol="FEMREC"/>
<gate name="-B16" symbol="FEMREC"/>
<gate name="-B17" symbol="FEMREC"/>
<gate name="-B18" symbol="FEMREC"/>
<gate name="-B19" symbol="FEMREC"/>
<gate name="-B20" symbol="FEMREC"/>
<gate name="-B21" symbol="FEMREC"/>
<gate name="-B22" symbol="FEMREC"/>
<gate name="-B23" symbol="FEMREC"/>
<gate name="-B24" symbol="FEMREC"/>
<gate name="-B25" symbol="FEMREC"/>
<gate name="-B26" symbol="FEMREC"/>
<gate name="-B27" symbol="FEMREC"/>
<gate name="-B28" symbol="FEMREC"/>
<gate name="-B29" symbol="FEMREC"/>
<gate name="-B30" symbol="FEMREC"/>
<gate name="-B31" symbol="FEMREC"/>
<gate name="-C2" symbol="FEMREC"/>
<gate name="-C3" symbol="FEMREC"/>
<gate name="-C4" symbol="FEMREC"/>
<gate name="-C5" symbol="FEMREC"/>
<gate name="-C6" symbol="FEMREC"/>
<gate name="-C7" symbol="FEMREC"/>
<gate name="-C8" symbol="FEMREC"/>
<gate name="-C9" symbol="FEMREC"/>
<gate name="-C10" symbol="FEMREC"/>
<gate name="-C11" symbol="FEMREC"/>
<gate name="-C12" symbol="FEMREC"/>
<gate name="-C13" symbol="FEMREC"/>
<gate name="-C14" symbol="FEMREC"/>
<gate name="-C15" symbol="FEMREC"/>
<gate name="-C16" symbol="FEMREC"/>
<gate name="-C17" symbol="FEMREC"/>
<gate name="-C18" symbol="FEMREC"/>
<gate name="-D2" symbol="FEMREC"/>
<gate name="-D3" symbol="FEMREC"/>
<gate name="-D4" symbol="FEMREC"/>
<gate name="-D5" symbol="FEMREC"/>
<gate name="-D6" symbol="FEMREC"/>
<gate name="-D7" symbol="FEMREC"/>
<gate name="-D8" symbol="FEMREC"/>
<gate name="-D9" symbol="FEMREC"/>
<gate name="-D10" symbol="FEMREC"/>
<gate name="-D11" symbol="FEMREC"/>
<gate name="-D12" symbol="FEMREC"/>
<gate name="-D13" symbol="FEMREC"/>
<gate name="-D14" symbol="FEMREC"/>
<gate name="-D15" symbol="FEMREC"/>
<gate name="-D16" symbol="FEMREC"/>
<gate name="-D17" symbol="FEMREC"/>
<gate name="-D18" symbol="FEMREC"/>
<gate name="-A1" symbol="FEMRVAL"/>
<gate name="-B1" symbol="FEMRVAL"/>
<gate name="-C1" symbol="FEMRVAL"/>
<gate name="-D1" symbol="FEMRVAL"/>
</gates>
<devices>
<device name="" package="ISA-16">
<connects>
<connect gate="-A1" pin="P" pad="A1"/>
<connect gate="-A10" pin="P" pad="A10"/>
<connect gate="-A11" pin="P" pad="A11"/>
<connect gate="-A12" pin="P" pad="A12"/>
<connect gate="-A13" pin="P" pad="A13"/>
<connect gate="-A14" pin="P" pad="A14"/>
<connect gate="-A15" pin="P" pad="A15"/>
<connect gate="-A16" pin="P" pad="A16"/>
<connect gate="-A17" pin="P" pad="A17"/>
<connect gate="-A18" pin="P" pad="A18"/>
<connect gate="-A19" pin="P" pad="A19"/>
<connect gate="-A2" pin="P" pad="A2"/>
<connect gate="-A20" pin="P" pad="A20"/>
<connect gate="-A21" pin="P" pad="A21"/>
<connect gate="-A22" pin="P" pad="A22"/>
<connect gate="-A23" pin="P" pad="A23"/>
<connect gate="-A24" pin="P" pad="A24"/>
<connect gate="-A25" pin="P" pad="A25"/>
<connect gate="-A26" pin="P" pad="A26"/>
<connect gate="-A27" pin="P" pad="A27"/>
<connect gate="-A28" pin="P" pad="A28"/>
<connect gate="-A29" pin="P" pad="A29"/>
<connect gate="-A3" pin="P" pad="A3"/>
<connect gate="-A30" pin="P" pad="A30"/>
<connect gate="-A31" pin="P" pad="A31"/>
<connect gate="-A4" pin="P" pad="A4"/>
<connect gate="-A5" pin="P" pad="A5"/>
<connect gate="-A6" pin="P" pad="A6"/>
<connect gate="-A7" pin="P" pad="A7"/>
<connect gate="-A8" pin="P" pad="A8"/>
<connect gate="-A9" pin="P" pad="A9"/>
<connect gate="-B1" pin="P" pad="B1"/>
<connect gate="-B10" pin="P" pad="B10"/>
<connect gate="-B11" pin="P" pad="B11"/>
<connect gate="-B12" pin="P" pad="B12"/>
<connect gate="-B13" pin="P" pad="B13"/>
<connect gate="-B14" pin="P" pad="B14"/>
<connect gate="-B15" pin="P" pad="B15"/>
<connect gate="-B16" pin="P" pad="B16"/>
<connect gate="-B17" pin="P" pad="B17"/>
<connect gate="-B18" pin="P" pad="B18"/>
<connect gate="-B19" pin="P" pad="B19"/>
<connect gate="-B2" pin="P" pad="B2"/>
<connect gate="-B20" pin="P" pad="B20"/>
<connect gate="-B21" pin="P" pad="B21"/>
<connect gate="-B22" pin="P" pad="B22"/>
<connect gate="-B23" pin="P" pad="B23"/>
<connect gate="-B24" pin="P" pad="B24"/>
<connect gate="-B25" pin="P" pad="B25"/>
<connect gate="-B26" pin="P" pad="B26"/>
<connect gate="-B27" pin="P" pad="B27"/>
<connect gate="-B28" pin="P" pad="B28"/>
<connect gate="-B29" pin="P" pad="B29"/>
<connect gate="-B3" pin="P" pad="B3"/>
<connect gate="-B30" pin="P" pad="B30"/>
<connect gate="-B31" pin="P" pad="B31"/>
<connect gate="-B4" pin="P" pad="B4"/>
<connect gate="-B5" pin="P" pad="B5"/>
<connect gate="-B6" pin="P" pad="B6"/>
<connect gate="-B7" pin="P" pad="B7"/>
<connect gate="-B8" pin="P" pad="B8"/>
<connect gate="-B9" pin="P" pad="B9"/>
<connect gate="-C1" pin="P" pad="C1"/>
<connect gate="-C10" pin="P" pad="C10"/>
<connect gate="-C11" pin="P" pad="C11"/>
<connect gate="-C12" pin="P" pad="C12"/>
<connect gate="-C13" pin="P" pad="C13"/>
<connect gate="-C14" pin="P" pad="C14"/>
<connect gate="-C15" pin="P" pad="C15"/>
<connect gate="-C16" pin="P" pad="C16"/>
<connect gate="-C17" pin="P" pad="C17"/>
<connect gate="-C18" pin="P" pad="C18"/>
<connect gate="-C2" pin="P" pad="C2"/>
<connect gate="-C3" pin="P" pad="C3"/>
<connect gate="-C4" pin="P" pad="C4"/>
<connect gate="-C5" pin="P" pad="C5"/>
<connect gate="-C6" pin="P" pad="C6"/>
<connect gate="-C7" pin="P" pad="C7"/>
<connect gate="-C8" pin="P" pad="C8"/>
<connect gate="-C9" pin="P" pad="C9"/>
<connect gate="-D1" pin="P" pad="D1"/>
<connect gate="-D10" pin="P" pad="D10"/>
<connect gate="-D11" pin="P" pad="D11"/>
<connect gate="-D12" pin="P" pad="D12"/>
<connect gate="-D13" pin="P" pad="D13"/>
<connect gate="-D14" pin="P" pad="D14"/>
<connect gate="-D15" pin="P" pad="D15"/>
<connect gate="-D16" pin="P" pad="D16"/>
<connect gate="-D17" pin="P" pad="D17"/>
<connect gate="-D18" pin="P" pad="D18"/>
<connect gate="-D2" pin="P" pad="D2"/>
<connect gate="-D3" pin="P" pad="D3"/>
<connect gate="-D4" pin="P" pad="D4"/>
<connect gate="-D5" pin="P" pad="D5"/>
<connect gate="-D6" pin="P" pad="D6"/>
<connect gate="-D7" pin="P" pad="D7"/>
<connect gate="-D8" pin="P" pad="D8"/>
<connect gate="-D9" pin="P" pad="D9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCI-SLOT" prefix="X" uservalue="yes">
<description>&lt;B&gt;PCI SLOT&lt;/B&gt;</description>
<gates>
<gate name="-A1" symbol="FEMRVAL"/>
<gate name="-A2" symbol="FEMREC"/>
<gate name="-A3" symbol="FEMREC"/>
<gate name="-A4" symbol="FEMREC"/>
<gate name="-A5" symbol="FEMREC"/>
<gate name="-A6" symbol="FEMREC"/>
<gate name="-A7" symbol="FEMREC"/>
<gate name="-A8" symbol="FEMREC"/>
<gate name="-A9" symbol="FEMREC"/>
<gate name="-A10" symbol="FEMREC"/>
<gate name="-A11" symbol="FEMREC"/>
<gate name="-A12" symbol="FEMREC"/>
<gate name="-A13" symbol="FEMREC"/>
<gate name="-A14" symbol="FEMREC"/>
<gate name="-A15" symbol="FEMREC"/>
<gate name="-A16" symbol="FEMREC"/>
<gate name="-A17" symbol="FEMREC"/>
<gate name="-A18" symbol="FEMREC"/>
<gate name="-A19" symbol="FEMREC"/>
<gate name="-A20" symbol="FEMREC"/>
<gate name="-A21" symbol="FEMREC"/>
<gate name="-A22" symbol="FEMREC"/>
<gate name="-A23" symbol="FEMREC"/>
<gate name="-A24" symbol="FEMREC"/>
<gate name="-A25" symbol="FEMREC"/>
<gate name="-A26" symbol="FEMREC"/>
<gate name="-A27" symbol="FEMREC"/>
<gate name="-A28" symbol="FEMREC"/>
<gate name="-A29" symbol="FEMREC"/>
<gate name="-A30" symbol="FEMREC"/>
<gate name="-A31" symbol="FEMREC"/>
<gate name="-A32" symbol="FEMREC"/>
<gate name="-A33" symbol="FEMREC"/>
<gate name="-A34" symbol="FEMREC"/>
<gate name="-A35" symbol="FEMREC"/>
<gate name="-A36" symbol="FEMREC"/>
<gate name="-A37" symbol="FEMREC"/>
<gate name="-A38" symbol="FEMREC"/>
<gate name="-A39" symbol="FEMREC"/>
<gate name="-A40" symbol="FEMREC"/>
<gate name="-A41" symbol="FEMREC"/>
<gate name="-A42" symbol="FEMREC"/>
<gate name="-A43" symbol="FEMREC"/>
<gate name="-A44" symbol="FEMREC"/>
<gate name="-A45" symbol="FEMREC"/>
<gate name="-A46" symbol="FEMREC"/>
<gate name="-A47" symbol="FEMREC"/>
<gate name="-A48" symbol="FEMREC"/>
<gate name="-A49" symbol="FEMREC"/>
<gate name="-A52" symbol="FEMREC"/>
<gate name="-A53" symbol="FEMREC"/>
<gate name="-A54" symbol="FEMREC"/>
<gate name="-A55" symbol="FEMREC"/>
<gate name="-A56" symbol="FEMREC"/>
<gate name="-A57" symbol="FEMREC"/>
<gate name="-A58" symbol="FEMREC"/>
<gate name="-A59" symbol="FEMREC"/>
<gate name="-A60" symbol="FEMREC"/>
<gate name="-A61" symbol="FEMREC"/>
<gate name="-A62" symbol="FEMREC"/>
<gate name="-B1" symbol="FEMRVAL"/>
<gate name="-B2" symbol="FEMREC"/>
<gate name="-B3" symbol="FEMREC"/>
<gate name="-B4" symbol="FEMREC"/>
<gate name="-B5" symbol="FEMREC"/>
<gate name="-B6" symbol="FEMREC"/>
<gate name="-B7" symbol="FEMREC"/>
<gate name="-B8" symbol="FEMREC"/>
<gate name="-B9" symbol="FEMREC"/>
<gate name="-B10" symbol="FEMREC"/>
<gate name="-B11" symbol="FEMREC"/>
<gate name="-B12" symbol="FEMREC"/>
<gate name="-B13" symbol="FEMREC"/>
<gate name="-B14" symbol="FEMREC"/>
<gate name="-B15" symbol="FEMREC"/>
<gate name="-B16" symbol="FEMREC"/>
<gate name="-B17" symbol="FEMREC"/>
<gate name="-B18" symbol="FEMREC"/>
<gate name="-B19" symbol="FEMREC"/>
<gate name="-B20" symbol="FEMREC"/>
<gate name="-B21" symbol="FEMREC"/>
<gate name="-B22" symbol="FEMREC"/>
<gate name="-B23" symbol="FEMREC"/>
<gate name="-B24" symbol="FEMREC"/>
<gate name="-B25" symbol="FEMREC"/>
<gate name="-B26" symbol="FEMREC"/>
<gate name="-B27" symbol="FEMREC"/>
<gate name="-B28" symbol="FEMREC"/>
<gate name="-B29" symbol="FEMREC"/>
<gate name="-B30" symbol="FEMREC"/>
<gate name="-B31" symbol="FEMREC"/>
<gate name="-B32" symbol="FEMREC"/>
<gate name="-B33" symbol="FEMREC"/>
<gate name="-B34" symbol="FEMREC"/>
<gate name="-B35" symbol="FEMREC"/>
<gate name="-B36" symbol="FEMREC"/>
<gate name="-B37" symbol="FEMREC"/>
<gate name="-B38" symbol="FEMREC"/>
<gate name="-B39" symbol="FEMREC"/>
<gate name="-B40" symbol="FEMREC"/>
<gate name="-B41" symbol="FEMREC"/>
<gate name="-B42" symbol="FEMREC"/>
<gate name="-B43" symbol="FEMREC"/>
<gate name="-B44" symbol="FEMREC"/>
<gate name="-B45" symbol="FEMREC"/>
<gate name="-B46" symbol="FEMREC"/>
<gate name="-B47" symbol="FEMREC"/>
<gate name="-B48" symbol="FEMREC"/>
<gate name="-B49" symbol="FEMREC"/>
<gate name="-B52" symbol="FEMREC"/>
<gate name="-B53" symbol="FEMREC"/>
<gate name="-B54" symbol="FEMREC"/>
<gate name="-B55" symbol="FEMREC"/>
<gate name="-B56" symbol="FEMREC"/>
<gate name="-B57" symbol="FEMREC"/>
<gate name="-B58" symbol="FEMREC"/>
<gate name="-B59" symbol="FEMREC"/>
<gate name="-B60" symbol="FEMREC"/>
<gate name="-B61" symbol="FEMREC"/>
<gate name="-B62" symbol="FEMREC"/>
</gates>
<devices>
<device name="" package="CON-PCI">
<connects>
<connect gate="-A1" pin="P" pad="A1"/>
<connect gate="-A10" pin="P" pad="A10"/>
<connect gate="-A11" pin="P" pad="A11"/>
<connect gate="-A12" pin="P" pad="A12"/>
<connect gate="-A13" pin="P" pad="A13"/>
<connect gate="-A14" pin="P" pad="A14"/>
<connect gate="-A15" pin="P" pad="A15"/>
<connect gate="-A16" pin="P" pad="A16"/>
<connect gate="-A17" pin="P" pad="A17"/>
<connect gate="-A18" pin="P" pad="A18"/>
<connect gate="-A19" pin="P" pad="A19"/>
<connect gate="-A2" pin="P" pad="A2"/>
<connect gate="-A20" pin="P" pad="A20"/>
<connect gate="-A21" pin="P" pad="A21"/>
<connect gate="-A22" pin="P" pad="A22"/>
<connect gate="-A23" pin="P" pad="A23"/>
<connect gate="-A24" pin="P" pad="A24"/>
<connect gate="-A25" pin="P" pad="A25"/>
<connect gate="-A26" pin="P" pad="A26"/>
<connect gate="-A27" pin="P" pad="A27"/>
<connect gate="-A28" pin="P" pad="A28"/>
<connect gate="-A29" pin="P" pad="A29"/>
<connect gate="-A3" pin="P" pad="A3"/>
<connect gate="-A30" pin="P" pad="A30"/>
<connect gate="-A31" pin="P" pad="A31"/>
<connect gate="-A32" pin="P" pad="A32"/>
<connect gate="-A33" pin="P" pad="A33"/>
<connect gate="-A34" pin="P" pad="A34"/>
<connect gate="-A35" pin="P" pad="A35"/>
<connect gate="-A36" pin="P" pad="A36"/>
<connect gate="-A37" pin="P" pad="A37"/>
<connect gate="-A38" pin="P" pad="A38"/>
<connect gate="-A39" pin="P" pad="A39"/>
<connect gate="-A4" pin="P" pad="A4"/>
<connect gate="-A40" pin="P" pad="A40"/>
<connect gate="-A41" pin="P" pad="A41"/>
<connect gate="-A42" pin="P" pad="A42"/>
<connect gate="-A43" pin="P" pad="A43"/>
<connect gate="-A44" pin="P" pad="A44"/>
<connect gate="-A45" pin="P" pad="A45"/>
<connect gate="-A46" pin="P" pad="A46"/>
<connect gate="-A47" pin="P" pad="A47"/>
<connect gate="-A48" pin="P" pad="A48"/>
<connect gate="-A49" pin="P" pad="A49"/>
<connect gate="-A5" pin="P" pad="A5"/>
<connect gate="-A52" pin="P" pad="A52"/>
<connect gate="-A53" pin="P" pad="A53"/>
<connect gate="-A54" pin="P" pad="A54"/>
<connect gate="-A55" pin="P" pad="A55"/>
<connect gate="-A56" pin="P" pad="A56"/>
<connect gate="-A57" pin="P" pad="A57"/>
<connect gate="-A58" pin="P" pad="A58"/>
<connect gate="-A59" pin="P" pad="A59"/>
<connect gate="-A6" pin="P" pad="A6"/>
<connect gate="-A60" pin="P" pad="A60"/>
<connect gate="-A61" pin="P" pad="A61"/>
<connect gate="-A62" pin="P" pad="A62"/>
<connect gate="-A7" pin="P" pad="A7"/>
<connect gate="-A8" pin="P" pad="A8"/>
<connect gate="-A9" pin="P" pad="A9"/>
<connect gate="-B1" pin="P" pad="B1"/>
<connect gate="-B10" pin="P" pad="B10"/>
<connect gate="-B11" pin="P" pad="B11"/>
<connect gate="-B12" pin="P" pad="B12"/>
<connect gate="-B13" pin="P" pad="B13"/>
<connect gate="-B14" pin="P" pad="B14"/>
<connect gate="-B15" pin="P" pad="B15"/>
<connect gate="-B16" pin="P" pad="B16"/>
<connect gate="-B17" pin="P" pad="B17"/>
<connect gate="-B18" pin="P" pad="B18"/>
<connect gate="-B19" pin="P" pad="B19"/>
<connect gate="-B2" pin="P" pad="B2"/>
<connect gate="-B20" pin="P" pad="B20"/>
<connect gate="-B21" pin="P" pad="B21"/>
<connect gate="-B22" pin="P" pad="B22"/>
<connect gate="-B23" pin="P" pad="B23"/>
<connect gate="-B24" pin="P" pad="B24"/>
<connect gate="-B25" pin="P" pad="B25"/>
<connect gate="-B26" pin="P" pad="B26"/>
<connect gate="-B27" pin="P" pad="B27"/>
<connect gate="-B28" pin="P" pad="B28"/>
<connect gate="-B29" pin="P" pad="B29"/>
<connect gate="-B3" pin="P" pad="B3"/>
<connect gate="-B30" pin="P" pad="B30"/>
<connect gate="-B31" pin="P" pad="B31"/>
<connect gate="-B32" pin="P" pad="B32"/>
<connect gate="-B33" pin="P" pad="B33"/>
<connect gate="-B34" pin="P" pad="B34"/>
<connect gate="-B35" pin="P" pad="B35"/>
<connect gate="-B36" pin="P" pad="B36"/>
<connect gate="-B37" pin="P" pad="B37"/>
<connect gate="-B38" pin="P" pad="B38"/>
<connect gate="-B39" pin="P" pad="B39"/>
<connect gate="-B4" pin="P" pad="B4"/>
<connect gate="-B40" pin="P" pad="B40"/>
<connect gate="-B41" pin="P" pad="B41"/>
<connect gate="-B42" pin="P" pad="B42"/>
<connect gate="-B43" pin="P" pad="B43"/>
<connect gate="-B44" pin="P" pad="B44"/>
<connect gate="-B45" pin="P" pad="B45"/>
<connect gate="-B46" pin="P" pad="B46"/>
<connect gate="-B47" pin="P" pad="B47"/>
<connect gate="-B48" pin="P" pad="B48"/>
<connect gate="-B49" pin="P" pad="B49"/>
<connect gate="-B5" pin="P" pad="B5"/>
<connect gate="-B52" pin="P" pad="B52"/>
<connect gate="-B53" pin="P" pad="B53"/>
<connect gate="-B54" pin="P" pad="B54"/>
<connect gate="-B55" pin="P" pad="B55"/>
<connect gate="-B56" pin="P" pad="B56"/>
<connect gate="-B57" pin="P" pad="B57"/>
<connect gate="-B58" pin="P" pad="B58"/>
<connect gate="-B59" pin="P" pad="B59"/>
<connect gate="-B6" pin="P" pad="B6"/>
<connect gate="-B60" pin="P" pad="B60"/>
<connect gate="-B61" pin="P" pad="B61"/>
<connect gate="-B62" pin="P" pad="B62"/>
<connect gate="-B7" pin="P" pad="B7"/>
<connect gate="-B8" pin="P" pad="B8"/>
<connect gate="-B9" pin="P" pad="B9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EISA-PAD" prefix="X" uservalue="yes">
<description>&lt;B&gt;EISA CARD CONNECTOR&lt;/B&gt;</description>
<gates>
<gate name="-CHCHK" symbol="MALE"/>
<gate name="-SD7" symbol="MALE"/>
<gate name="-SD6" symbol="MALE"/>
<gate name="-SD5" symbol="MALE"/>
<gate name="-SD4" symbol="MALE"/>
<gate name="-SD3" symbol="MALE"/>
<gate name="-SD2" symbol="MALE"/>
<gate name="-SD1" symbol="MALE"/>
<gate name="-SD0" symbol="MALE"/>
<gate name="-CHRDY" symbol="MALE"/>
<gate name="-AEN" symbol="MALE"/>
<gate name="-SA19" symbol="MALE"/>
<gate name="-SA18" symbol="MALE"/>
<gate name="-SA17" symbol="MALE"/>
<gate name="-SA16" symbol="MALE"/>
<gate name="-SA15" symbol="MALE"/>
<gate name="-SA14" symbol="MALE"/>
<gate name="-SA13" symbol="MALE"/>
<gate name="-SA12" symbol="MALE"/>
<gate name="-SA11" symbol="MALE"/>
<gate name="-SA10" symbol="MALE"/>
<gate name="-SA9" symbol="MALE"/>
<gate name="-SA8" symbol="MALE"/>
<gate name="-SA7" symbol="MALE"/>
<gate name="-SA6" symbol="MALE"/>
<gate name="-SA5" symbol="MALE"/>
<gate name="-SA4" symbol="MALE"/>
<gate name="-SA3" symbol="MALE"/>
<gate name="-SA2" symbol="MALE"/>
<gate name="-SA1" symbol="MALE"/>
<gate name="-SA0" symbol="MALE"/>
<gate name="GND11" symbol="GND"/>
<gate name="-RESV10" symbol="MALE"/>
<gate name="+5V5" symbol="+5V"/>
<gate name="-IRQ2" symbol="MALE"/>
<gate name="-5V0" symbol="-5V"/>
<gate name="-DRQ2" symbol="MALE"/>
<gate name="-12V0" symbol="-12V"/>
<gate name="-NOWS" symbol="MALE"/>
<gate name="+12V0" symbol="+12V"/>
<gate name="GND12" symbol="GND"/>
<gate name="-SMWTC" symbol="MALE"/>
<gate name="-SMRDC" symbol="MALE"/>
<gate name="-IOWC" symbol="MALE"/>
<gate name="-IORC" symbol="MALE"/>
<gate name="-DAK3" symbol="MALE"/>
<gate name="-DRQ3" symbol="MALE"/>
<gate name="-DAK1" symbol="MALE"/>
<gate name="-DRQ1" symbol="MALE"/>
<gate name="-REFRESH" symbol="MALE"/>
<gate name="-BLCK" symbol="MALE"/>
<gate name="-IRQ7" symbol="MALE"/>
<gate name="-IRQ6" symbol="MALE"/>
<gate name="-IRQ5" symbol="MALE"/>
<gate name="-IRQ4" symbol="MALE"/>
<gate name="-IRQ3" symbol="MALE"/>
<gate name="-DAK2" symbol="MALE"/>
<gate name="-TC" symbol="MALE"/>
<gate name="-BALE" symbol="MALE"/>
<gate name="+5V6" symbol="+5V"/>
<gate name="-OSC" symbol="MALE"/>
<gate name="GND13" symbol="GND"/>
<gate name="-CMD" symbol="MALE"/>
<gate name="-START" symbol="MALE"/>
<gate name="-EXRDY" symbol="MALE"/>
<gate name="-EX32" symbol="MALE"/>
<gate name="GND0" symbol="GND"/>
<gate name="-EX16" symbol="MALE"/>
<gate name="-SLBURST" symbol="MALE"/>
<gate name="-MSBURST" symbol="MALE"/>
<gate name="-W/R" symbol="MALE"/>
<gate name="GND1" symbol="GND"/>
<gate name="-RESERV1" symbol="RESERV"/>
<gate name="-RESERV2" symbol="RESERV"/>
<gate name="-RESERV3" symbol="RESERV"/>
<gate name="GND2" symbol="GND"/>
<gate name="-BE1" symbol="MALE"/>
<gate name="-LA31" symbol="MALE"/>
<gate name="GND3" symbol="GND"/>
<gate name="-LA30" symbol="MALE"/>
<gate name="-LA28" symbol="MALE"/>
<gate name="-LA27" symbol="MALE"/>
<gate name="-LA25" symbol="MALE"/>
<gate name="GND4" symbol="GND"/>
<gate name="-LA15" symbol="MALE"/>
<gate name="-LA13" symbol="MALE"/>
<gate name="-LA12" symbol="MALE"/>
<gate name="-LA11" symbol="MALE"/>
<gate name="GND5" symbol="GND"/>
<gate name="-LA9" symbol="MALE"/>
<gate name="GND6" symbol="GND"/>
<gate name="+5V0" symbol="+5V"/>
<gate name="+5V1" symbol="+5V"/>
<gate name="-RESERV4" symbol="RESERV"/>
<gate name="-RESERV5" symbol="RESERV"/>
<gate name="-RESERV6" symbol="RESERV"/>
<gate name="-RESERV7" symbol="RESERV"/>
<gate name="+12V" symbol="+12V"/>
<gate name="-M/IO" symbol="MALE"/>
<gate name="-LOCK" symbol="MALE"/>
<gate name="-RESERV8" symbol="RESERV"/>
<gate name="GND7" symbol="GND"/>
<gate name="-RESERV9" symbol="RESERV"/>
<gate name="-BE3" symbol="MALE"/>
<gate name="-BE2" symbol="MALE"/>
<gate name="-BE0" symbol="MALE"/>
<gate name="GND8" symbol="GND"/>
<gate name="+5V2" symbol="+5V"/>
<gate name="-LA29" symbol="MALE"/>
<gate name="GND9" symbol="GND"/>
<gate name="-LA26" symbol="MALE"/>
<gate name="-LA24" symbol="MALE"/>
<gate name="-LA16" symbol="MALE"/>
<gate name="-LA14" symbol="MALE"/>
<gate name="+5V3" symbol="+5V"/>
<gate name="+5V4" symbol="+5V"/>
<gate name="GND10" symbol="GND"/>
<gate name="-LA10" symbol="MALE"/>
<gate name="-SBHE" symbol="MALE"/>
<gate name="-LA23" symbol="MALE"/>
<gate name="-LA22" symbol="MALE"/>
<gate name="-LA21" symbol="MALE"/>
<gate name="-LA20" symbol="MALE"/>
<gate name="-LA19" symbol="MALE"/>
<gate name="-LA18" symbol="MALE"/>
<gate name="-LA17" symbol="MALE"/>
<gate name="-MRDC" symbol="MALE"/>
<gate name="-MWTC" symbol="MALE"/>
<gate name="-SD8" symbol="MALE"/>
<gate name="-SD9" symbol="MALE"/>
<gate name="-SD10" symbol="MALE"/>
<gate name="-SD11" symbol="MALE"/>
<gate name="-SD12" symbol="MALE"/>
<gate name="-SD13" symbol="MALE"/>
<gate name="-SD14" symbol="MALE"/>
<gate name="-SD15" symbol="MALE"/>
<gate name="-M16" symbol="MALE"/>
<gate name="-IO16" symbol="MALE"/>
<gate name="-IRQ10" symbol="MALE"/>
<gate name="-IRQ11" symbol="MALE"/>
<gate name="-IRQ12" symbol="MALE"/>
<gate name="-IRQ13" symbol="MALE"/>
<gate name="-IRQ14" symbol="MALE"/>
<gate name="-DAK0" symbol="MALE"/>
<gate name="-DRQ0" symbol="MALE"/>
<gate name="-DAK5" symbol="MALE"/>
<gate name="-DRQ5" symbol="MALE"/>
<gate name="-DAK6" symbol="MALE"/>
<gate name="-DRQ6" symbol="MALE"/>
<gate name="-DAK7" symbol="MALE"/>
<gate name="-DRQ7" symbol="MALE"/>
<gate name="+5V10" symbol="+5V"/>
<gate name="MASTER16" symbol="MALE"/>
<gate name="GND20" symbol="GND"/>
<gate name="-LA7" symbol="MALE"/>
<gate name="GND14" symbol="GND"/>
<gate name="-LA4" symbol="MALE"/>
<gate name="-LA3" symbol="MALE"/>
<gate name="GND15" symbol="GND"/>
<gate name="-SD17" symbol="MALE"/>
<gate name="-SD19" symbol="MALE"/>
<gate name="-SD20" symbol="MALE"/>
<gate name="-SD22" symbol="MALE"/>
<gate name="GND16" symbol="GND"/>
<gate name="-SD25" symbol="MALE"/>
<gate name="-SD26" symbol="MALE"/>
<gate name="-SD28" symbol="MALE"/>
<gate name="GND17" symbol="GND"/>
<gate name="-SD30" symbol="MALE"/>
<gate name="-SD31" symbol="MALE"/>
<gate name="-MREQX" symbol="MALE"/>
<gate name="-LA8" symbol="MALE"/>
<gate name="-LA6" symbol="MALE"/>
<gate name="-LA5" symbol="MALE"/>
<gate name="+5V7" symbol="+5V"/>
<gate name="-LA2" symbol="MALE"/>
<gate name="-SD16" symbol="MALE"/>
<gate name="-SD18" symbol="MALE"/>
<gate name="GND18" symbol="GND"/>
<gate name="-SD21" symbol="MALE"/>
<gate name="-SD23" symbol="MALE"/>
<gate name="-SD24" symbol="MALE"/>
<gate name="GND19" symbol="GND"/>
<gate name="-SD27" symbol="MALE"/>
<gate name="-SD29" symbol="MALE"/>
<gate name="+5V8" symbol="+5V"/>
<gate name="+5V9" symbol="+5V"/>
<gate name="-MAKX" symbol="MALE"/>
</gates>
<devices>
<device name="" package="EISA-BRD">
<connects>
<connect gate="+12V" pin="+12V" pad="F9"/>
<connect gate="+12V0" pin="+12V" pad="B9"/>
<connect gate="+5V0" pin="+5V" pad="F2"/>
<connect gate="+5V1" pin="+5V" pad="F3"/>
<connect gate="+5V10" pin="+5V" pad="D16"/>
<connect gate="+5V2" pin="+5V" pad="F20"/>
<connect gate="+5V3" pin="+5V" pad="F28"/>
<connect gate="+5V4" pin="+5V" pad="F29"/>
<connect gate="+5V5" pin="+5V" pad="B3"/>
<connect gate="+5V6" pin="+5V" pad="B29"/>
<connect gate="+5V7" pin="+5V" pad="H4"/>
<connect gate="+5V8" pin="+5V" pad="H17"/>
<connect gate="+5V9" pin="+5V" pad="H18"/>
<connect gate="-12V0" pin="-12V" pad="B7"/>
<connect gate="-5V0" pin="-5V" pad="B5"/>
<connect gate="-AEN" pin="P" pad="A11"/>
<connect gate="-BALE" pin="P" pad="B28"/>
<connect gate="-BE0" pin="P" pad="F18"/>
<connect gate="-BE1" pin="P" pad="E17"/>
<connect gate="-BE2" pin="P" pad="F17"/>
<connect gate="-BE3" pin="P" pad="F15"/>
<connect gate="-BLCK" pin="P" pad="B20"/>
<connect gate="-CHCHK" pin="P" pad="A1"/>
<connect gate="-CHRDY" pin="P" pad="A10"/>
<connect gate="-CMD" pin="P" pad="E1"/>
<connect gate="-DAK0" pin="P" pad="D8"/>
<connect gate="-DAK1" pin="P" pad="B17"/>
<connect gate="-DAK2" pin="P" pad="B26"/>
<connect gate="-DAK3" pin="P" pad="B15"/>
<connect gate="-DAK5" pin="P" pad="D10"/>
<connect gate="-DAK6" pin="P" pad="D12"/>
<connect gate="-DAK7" pin="P" pad="D14"/>
<connect gate="-DRQ0" pin="P" pad="D9"/>
<connect gate="-DRQ1" pin="P" pad="B18"/>
<connect gate="-DRQ2" pin="P" pad="B6"/>
<connect gate="-DRQ3" pin="P" pad="B16"/>
<connect gate="-DRQ5" pin="P" pad="D11"/>
<connect gate="-DRQ6" pin="P" pad="D13"/>
<connect gate="-DRQ7" pin="P" pad="D15"/>
<connect gate="-EX16" pin="P" pad="E7"/>
<connect gate="-EX32" pin="P" pad="E4"/>
<connect gate="-EXRDY" pin="P" pad="E3"/>
<connect gate="-IO16" pin="P" pad="D2"/>
<connect gate="-IORC" pin="P" pad="B14"/>
<connect gate="-IOWC" pin="P" pad="B13"/>
<connect gate="-IRQ10" pin="P" pad="D3"/>
<connect gate="-IRQ11" pin="P" pad="D4"/>
<connect gate="-IRQ12" pin="P" pad="D5"/>
<connect gate="-IRQ13" pin="P" pad="D6"/>
<connect gate="-IRQ14" pin="P" pad="D7"/>
<connect gate="-IRQ2" pin="P" pad="B4"/>
<connect gate="-IRQ3" pin="P" pad="B25"/>
<connect gate="-IRQ4" pin="P" pad="B24"/>
<connect gate="-IRQ5" pin="P" pad="B23"/>
<connect gate="-IRQ6" pin="P" pad="B22"/>
<connect gate="-IRQ7" pin="P" pad="B21"/>
<connect gate="-LA10" pin="P" pad="F31"/>
<connect gate="-LA11" pin="P" pad="E29"/>
<connect gate="-LA12" pin="P" pad="E28"/>
<connect gate="-LA13" pin="P" pad="E27"/>
<connect gate="-LA14" pin="P" pad="F27"/>
<connect gate="-LA15" pin="P" pad="E26"/>
<connect gate="-LA16" pin="P" pad="F26"/>
<connect gate="-LA17" pin="P" pad="C8"/>
<connect gate="-LA18" pin="P" pad="C7"/>
<connect gate="-LA19" pin="P" pad="C6"/>
<connect gate="-LA2" pin="P" pad="H5"/>
<connect gate="-LA20" pin="P" pad="C5"/>
<connect gate="-LA21" pin="P" pad="C4"/>
<connect gate="-LA22" pin="P" pad="C3"/>
<connect gate="-LA23" pin="P" pad="C2"/>
<connect gate="-LA24" pin="P" pad="F24"/>
<connect gate="-LA25" pin="P" pad="E23"/>
<connect gate="-LA26" pin="P" pad="F23"/>
<connect gate="-LA27" pin="P" pad="E22"/>
<connect gate="-LA28" pin="P" pad="E21"/>
<connect gate="-LA29" pin="P" pad="F21"/>
<connect gate="-LA3" pin="P" pad="G4"/>
<connect gate="-LA30" pin="P" pad="E20"/>
<connect gate="-LA31" pin="P" pad="E18"/>
<connect gate="-LA4" pin="P" pad="G3"/>
<connect gate="-LA5" pin="P" pad="H3"/>
<connect gate="-LA6" pin="P" pad="H2"/>
<connect gate="-LA7" pin="P" pad="G1"/>
<connect gate="-LA8" pin="P" pad="H1"/>
<connect gate="-LA9" pin="P" pad="E31"/>
<connect gate="-LOCK" pin="P" pad="F11"/>
<connect gate="-M/IO" pin="P" pad="F10"/>
<connect gate="-M16" pin="P" pad="D1"/>
<connect gate="-MAKX" pin="P" pad="H19"/>
<connect gate="-MRDC" pin="P" pad="C9"/>
<connect gate="-MREQX" pin="P" pad="G19"/>
<connect gate="-MSBURST" pin="P" pad="E9"/>
<connect gate="-MWTC" pin="P" pad="C10"/>
<connect gate="-NOWS" pin="P" pad="B8"/>
<connect gate="-OSC" pin="P" pad="B30"/>
<connect gate="-REFRESH" pin="P" pad="B19"/>
<connect gate="-RESERV1" pin="RSV" pad="E12"/>
<connect gate="-RESERV2" pin="RSV" pad="E13"/>
<connect gate="-RESERV3" pin="RSV" pad="E14"/>
<connect gate="-RESERV4" pin="RSV" pad="F4"/>
<connect gate="-RESERV5" pin="RSV" pad="F5"/>
<connect gate="-RESERV6" pin="RSV" pad="F7"/>
<connect gate="-RESERV7" pin="RSV" pad="F8"/>
<connect gate="-RESERV8" pin="RSV" pad="F12"/>
<connect gate="-RESERV9" pin="RSV" pad="F14"/>
<connect gate="-RESV10" pin="P" pad="B2"/>
<connect gate="-SA0" pin="P" pad="A31"/>
<connect gate="-SA1" pin="P" pad="A30"/>
<connect gate="-SA10" pin="P" pad="A21"/>
<connect gate="-SA11" pin="P" pad="A20"/>
<connect gate="-SA12" pin="P" pad="A19"/>
<connect gate="-SA13" pin="P" pad="A18"/>
<connect gate="-SA14" pin="P" pad="A17"/>
<connect gate="-SA15" pin="P" pad="A16"/>
<connect gate="-SA16" pin="P" pad="A15"/>
<connect gate="-SA17" pin="P" pad="A14"/>
<connect gate="-SA18" pin="P" pad="A13"/>
<connect gate="-SA19" pin="P" pad="A12"/>
<connect gate="-SA2" pin="P" pad="A29"/>
<connect gate="-SA3" pin="P" pad="A28"/>
<connect gate="-SA4" pin="P" pad="A27"/>
<connect gate="-SA5" pin="P" pad="A26"/>
<connect gate="-SA6" pin="P" pad="A25"/>
<connect gate="-SA7" pin="P" pad="A24"/>
<connect gate="-SA8" pin="P" pad="A23"/>
<connect gate="-SA9" pin="P" pad="A22"/>
<connect gate="-SBHE" pin="P" pad="C1"/>
<connect gate="-SD0" pin="P" pad="A9"/>
<connect gate="-SD1" pin="P" pad="A8"/>
<connect gate="-SD10" pin="P" pad="C13"/>
<connect gate="-SD11" pin="P" pad="C14"/>
<connect gate="-SD12" pin="P" pad="C15"/>
<connect gate="-SD13" pin="P" pad="C16"/>
<connect gate="-SD14" pin="P" pad="C17"/>
<connect gate="-SD15" pin="P" pad="C18"/>
<connect gate="-SD16" pin="P" pad="H7"/>
<connect gate="-SD17" pin="P" pad="G7"/>
<connect gate="-SD18" pin="P" pad="H8"/>
<connect gate="-SD19" pin="P" pad="G8"/>
<connect gate="-SD2" pin="P" pad="A7"/>
<connect gate="-SD20" pin="P" pad="G9"/>
<connect gate="-SD21" pin="P" pad="H10"/>
<connect gate="-SD22" pin="P" pad="G10"/>
<connect gate="-SD23" pin="P" pad="H11"/>
<connect gate="-SD24" pin="P" pad="H12"/>
<connect gate="-SD25" pin="P" pad="G12"/>
<connect gate="-SD26" pin="P" pad="G13"/>
<connect gate="-SD27" pin="P" pad="H14"/>
<connect gate="-SD28" pin="P" pad="G14"/>
<connect gate="-SD29" pin="P" pad="H16"/>
<connect gate="-SD3" pin="P" pad="A6"/>
<connect gate="-SD30" pin="P" pad="G17"/>
<connect gate="-SD31" pin="P" pad="G18"/>
<connect gate="-SD4" pin="P" pad="A5"/>
<connect gate="-SD5" pin="P" pad="A4"/>
<connect gate="-SD6" pin="P" pad="A3"/>
<connect gate="-SD7" pin="P" pad="A2"/>
<connect gate="-SD8" pin="P" pad="C11"/>
<connect gate="-SD9" pin="P" pad="C12"/>
<connect gate="-SLBURST" pin="P" pad="E8"/>
<connect gate="-SMRDC" pin="P" pad="B12"/>
<connect gate="-SMWTC" pin="P" pad="B11"/>
<connect gate="-START" pin="P" pad="E2"/>
<connect gate="-TC" pin="P" pad="B27"/>
<connect gate="-W/R" pin="P" pad="E10"/>
<connect gate="GND0" pin="GND" pad="E5"/>
<connect gate="GND1" pin="GND" pad="E11"/>
<connect gate="GND10" pin="GND" pad="F30"/>
<connect gate="GND11" pin="GND" pad="B1"/>
<connect gate="GND12" pin="GND" pad="B10"/>
<connect gate="GND13" pin="GND" pad="B31"/>
<connect gate="GND14" pin="GND" pad="G2"/>
<connect gate="GND15" pin="GND" pad="G5"/>
<connect gate="GND16" pin="GND" pad="G11"/>
<connect gate="GND17" pin="GND" pad="G16"/>
<connect gate="GND18" pin="GND" pad="H9"/>
<connect gate="GND19" pin="GND" pad="H13"/>
<connect gate="GND2" pin="GND" pad="E15"/>
<connect gate="GND20" pin="GND" pad="D18"/>
<connect gate="GND3" pin="GND" pad="E19"/>
<connect gate="GND4" pin="GND" pad="E24"/>
<connect gate="GND5" pin="GND" pad="E30"/>
<connect gate="GND6" pin="GND" pad="F1"/>
<connect gate="GND7" pin="GND" pad="F13"/>
<connect gate="GND8" pin="GND" pad="F19"/>
<connect gate="GND9" pin="GND" pad="F22"/>
<connect gate="MASTER16" pin="P" pad="D17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EISA-SLOT" prefix="X" uservalue="yes">
<description>&lt;b&gt;EISA SLOT&lt;/b&gt;</description>
<gates>
<gate name="-CHCHK" symbol="FEMREC"/>
<gate name="-SD7" symbol="FEMREC"/>
<gate name="-SD6" symbol="FEMREC"/>
<gate name="-SD5" symbol="FEMREC"/>
<gate name="-SD4" symbol="FEMREC"/>
<gate name="-SD3" symbol="FEMREC"/>
<gate name="-SD2" symbol="FEMREC"/>
<gate name="-SD1" symbol="FEMREC"/>
<gate name="-SD0" symbol="FEMREC"/>
<gate name="-CHRDY" symbol="FEMREC"/>
<gate name="-AEN" symbol="FEMREC"/>
<gate name="-SA19" symbol="FEMREC"/>
<gate name="-SA18" symbol="FEMREC"/>
<gate name="-SA17" symbol="FEMREC"/>
<gate name="-SA16" symbol="FEMREC"/>
<gate name="-SA15" symbol="FEMREC"/>
<gate name="-SA14" symbol="FEMREC"/>
<gate name="-SA13" symbol="FEMREC"/>
<gate name="-SA12" symbol="FEMREC"/>
<gate name="-SA11" symbol="FEMREC"/>
<gate name="-SA10" symbol="FEMREC"/>
<gate name="-SA9" symbol="FEMREC"/>
<gate name="-SA8" symbol="FEMREC"/>
<gate name="-SA7" symbol="FEMREC"/>
<gate name="-SA6" symbol="FEMREC"/>
<gate name="-SA5" symbol="FEMREC"/>
<gate name="-SA4" symbol="FEMREC"/>
<gate name="-SA3" symbol="FEMREC"/>
<gate name="-SA2" symbol="FEMREC"/>
<gate name="-SA1" symbol="FEMREC"/>
<gate name="-SA0" symbol="FEMREC"/>
<gate name="GND11" symbol="GND"/>
<gate name="-RESV10" symbol="FEMREC"/>
<gate name="+5V5" symbol="+5V"/>
<gate name="-IRQ2" symbol="FEMREC"/>
<gate name="-5V0" symbol="-5V"/>
<gate name="-DRQ2" symbol="FEMREC"/>
<gate name="-12V0" symbol="-12V"/>
<gate name="-NOWS" symbol="FEMREC"/>
<gate name="+12V0" symbol="+12V"/>
<gate name="GND12" symbol="GND"/>
<gate name="-SMWTC" symbol="FEMREC"/>
<gate name="-SMRDC" symbol="FEMREC"/>
<gate name="-IOWC" symbol="FEMREC"/>
<gate name="-IORC" symbol="FEMREC"/>
<gate name="-DAK3" symbol="FEMREC"/>
<gate name="-DRQ3" symbol="FEMREC"/>
<gate name="-DAK1" symbol="FEMREC"/>
<gate name="-DRQ1" symbol="FEMREC"/>
<gate name="-REFRESH" symbol="FEMREC"/>
<gate name="-BLCK" symbol="FEMREC"/>
<gate name="-IRQ7" symbol="FEMREC"/>
<gate name="-IRQ6" symbol="FEMREC"/>
<gate name="-IRQ5" symbol="FEMREC"/>
<gate name="-IRQ4" symbol="FEMREC"/>
<gate name="-IRQ3" symbol="FEMREC"/>
<gate name="-DAK2" symbol="FEMREC"/>
<gate name="-TC" symbol="FEMREC"/>
<gate name="-BALE" symbol="FEMREC"/>
<gate name="+5V6" symbol="+5V"/>
<gate name="-OSC" symbol="FEMREC"/>
<gate name="GND13" symbol="GND"/>
<gate name="-CMD" symbol="FEMREC"/>
<gate name="-START" symbol="FEMREC"/>
<gate name="-EXRDY" symbol="FEMREC"/>
<gate name="-EX32" symbol="FEMREC"/>
<gate name="GND0" symbol="GND"/>
<gate name="-EX16" symbol="FEMREC"/>
<gate name="-SLBURST" symbol="FEMREC"/>
<gate name="-MSBURST" symbol="FEMREC"/>
<gate name="-W/R" symbol="FEMREC"/>
<gate name="GND1" symbol="GND"/>
<gate name="-RESERV1" symbol="RESERV"/>
<gate name="-RESERV2" symbol="RESERV"/>
<gate name="-RESERV3" symbol="RESERV"/>
<gate name="GND2" symbol="GND"/>
<gate name="-BE1" symbol="FEMREC"/>
<gate name="-LA31" symbol="FEMREC"/>
<gate name="GND3" symbol="GND"/>
<gate name="-LA30" symbol="FEMREC"/>
<gate name="-LA28" symbol="FEMREC"/>
<gate name="-LA27" symbol="FEMREC"/>
<gate name="-LA25" symbol="FEMREC"/>
<gate name="GND4" symbol="GND"/>
<gate name="-LA15" symbol="FEMREC"/>
<gate name="-LA13" symbol="FEMREC"/>
<gate name="-LA12" symbol="FEMREC"/>
<gate name="-LA11" symbol="FEMREC"/>
<gate name="GND5" symbol="GND"/>
<gate name="-LA9" symbol="FEMREC"/>
<gate name="GND6" symbol="GND"/>
<gate name="+5V0" symbol="+5V"/>
<gate name="+5V1" symbol="+5V"/>
<gate name="-RESERV4" symbol="RESERV"/>
<gate name="-RESERV5" symbol="RESERV"/>
<gate name="-RESERV6" symbol="RESERV"/>
<gate name="-RESERV7" symbol="RESERV"/>
<gate name="+12V" symbol="+12V"/>
<gate name="-M/IO" symbol="FEMREC"/>
<gate name="-LOCK" symbol="FEMREC"/>
<gate name="-RESERV8" symbol="RESERV"/>
<gate name="GND7" symbol="GND"/>
<gate name="-RESERV9" symbol="RESERV"/>
<gate name="-BE3" symbol="FEMREC"/>
<gate name="-BE2" symbol="FEMREC"/>
<gate name="-BE0" symbol="FEMREC"/>
<gate name="GND8" symbol="GND"/>
<gate name="+5V2" symbol="+5V"/>
<gate name="-LA29" symbol="FEMREC"/>
<gate name="GND9" symbol="GND"/>
<gate name="-LA26" symbol="FEMREC"/>
<gate name="-LA24" symbol="FEMREC"/>
<gate name="-LA16" symbol="FEMREC"/>
<gate name="-LA14" symbol="FEMREC"/>
<gate name="+5V3" symbol="+5V"/>
<gate name="+5V4" symbol="+5V"/>
<gate name="GND10" symbol="GND"/>
<gate name="-LA10" symbol="FEMREC"/>
<gate name="-SBHE" symbol="FEMREC"/>
<gate name="-LA23" symbol="FEMREC"/>
<gate name="-LA22" symbol="FEMREC"/>
<gate name="-LA21" symbol="FEMREC"/>
<gate name="-LA20" symbol="FEMREC"/>
<gate name="-LA19" symbol="FEMREC"/>
<gate name="-LA18" symbol="FEMREC"/>
<gate name="-LA17" symbol="FEMREC"/>
<gate name="-MRDC" symbol="FEMREC"/>
<gate name="-MWTC" symbol="FEMREC"/>
<gate name="-SD8" symbol="FEMREC"/>
<gate name="-SD9" symbol="FEMREC"/>
<gate name="-SD10" symbol="FEMREC"/>
<gate name="-SD11" symbol="FEMREC"/>
<gate name="-SD12" symbol="FEMREC"/>
<gate name="-SD13" symbol="FEMREC"/>
<gate name="-SD14" symbol="FEMREC"/>
<gate name="-SD15" symbol="FEMREC"/>
<gate name="-M16" symbol="FEMREC"/>
<gate name="-IO16" symbol="FEMREC"/>
<gate name="-IRQ10" symbol="FEMREC"/>
<gate name="-IRQ11" symbol="FEMREC"/>
<gate name="-IRQ12" symbol="FEMREC"/>
<gate name="-IRQ13" symbol="FEMREC"/>
<gate name="-IRQ14" symbol="FEMREC"/>
<gate name="-DAK0" symbol="FEMREC"/>
<gate name="-DRQ0" symbol="FEMREC"/>
<gate name="-DAK5" symbol="FEMREC"/>
<gate name="-DRQ5" symbol="FEMREC"/>
<gate name="-DAK6" symbol="FEMREC"/>
<gate name="-DRQ6" symbol="FEMREC"/>
<gate name="-DAK7" symbol="FEMREC"/>
<gate name="-DRQ7" symbol="FEMREC"/>
<gate name="+5V10" symbol="+5V"/>
<gate name="MASTER16" symbol="FEMREC"/>
<gate name="GND20" symbol="GND"/>
<gate name="-LA7" symbol="FEMREC"/>
<gate name="GND14" symbol="GND"/>
<gate name="-LA4" symbol="FEMREC"/>
<gate name="-LA3" symbol="FEMREC"/>
<gate name="GND15" symbol="GND"/>
<gate name="-SD17" symbol="FEMREC"/>
<gate name="-SD19" symbol="FEMREC"/>
<gate name="-SD20" symbol="FEMREC"/>
<gate name="-SD22" symbol="FEMREC"/>
<gate name="GND16" symbol="GND"/>
<gate name="-SD25" symbol="FEMREC"/>
<gate name="-SD26" symbol="FEMREC"/>
<gate name="-SD28" symbol="FEMREC"/>
<gate name="GND17" symbol="GND"/>
<gate name="-SD30" symbol="FEMREC"/>
<gate name="-SD31" symbol="FEMREC"/>
<gate name="-MREQX" symbol="FEMREC"/>
<gate name="-LA8" symbol="FEMREC"/>
<gate name="-LA6" symbol="FEMREC"/>
<gate name="-LA5" symbol="FEMREC"/>
<gate name="+5V7" symbol="+5V"/>
<gate name="-LA2" symbol="FEMREC"/>
<gate name="-SD16" symbol="FEMREC"/>
<gate name="-SD18" symbol="FEMREC"/>
<gate name="GND18" symbol="GND"/>
<gate name="-SD21" symbol="FEMREC"/>
<gate name="-SD23" symbol="FEMREC"/>
<gate name="-SD24" symbol="FEMREC"/>
<gate name="GND19" symbol="GND"/>
<gate name="-SD27" symbol="FEMREC"/>
<gate name="-SD29" symbol="FEMREC"/>
<gate name="+5V8" symbol="+5V"/>
<gate name="+5V9" symbol="+5V"/>
<gate name="-MAKX" symbol="FEMREC"/>
</gates>
<devices>
<device name="" package="EISA-188">
<connects>
<connect gate="+12V" pin="+12V" pad="F9"/>
<connect gate="+12V0" pin="+12V" pad="B9"/>
<connect gate="+5V0" pin="+5V" pad="F2"/>
<connect gate="+5V1" pin="+5V" pad="F3"/>
<connect gate="+5V10" pin="+5V" pad="D16"/>
<connect gate="+5V2" pin="+5V" pad="F20"/>
<connect gate="+5V3" pin="+5V" pad="F28"/>
<connect gate="+5V4" pin="+5V" pad="F29"/>
<connect gate="+5V5" pin="+5V" pad="B3"/>
<connect gate="+5V6" pin="+5V" pad="B29"/>
<connect gate="+5V7" pin="+5V" pad="H4"/>
<connect gate="+5V8" pin="+5V" pad="H17"/>
<connect gate="+5V9" pin="+5V" pad="H18"/>
<connect gate="-12V0" pin="-12V" pad="B7"/>
<connect gate="-5V0" pin="-5V" pad="B5"/>
<connect gate="-AEN" pin="P" pad="A11"/>
<connect gate="-BALE" pin="P" pad="B28"/>
<connect gate="-BE0" pin="P" pad="F18"/>
<connect gate="-BE1" pin="P" pad="E17"/>
<connect gate="-BE2" pin="P" pad="F17"/>
<connect gate="-BE3" pin="P" pad="F15"/>
<connect gate="-BLCK" pin="P" pad="B20"/>
<connect gate="-CHCHK" pin="P" pad="A1"/>
<connect gate="-CHRDY" pin="P" pad="A10"/>
<connect gate="-CMD" pin="P" pad="E1"/>
<connect gate="-DAK0" pin="P" pad="D8"/>
<connect gate="-DAK1" pin="P" pad="B17"/>
<connect gate="-DAK2" pin="P" pad="B26"/>
<connect gate="-DAK3" pin="P" pad="B15"/>
<connect gate="-DAK5" pin="P" pad="D10"/>
<connect gate="-DAK6" pin="P" pad="D12"/>
<connect gate="-DAK7" pin="P" pad="D14"/>
<connect gate="-DRQ0" pin="P" pad="D9"/>
<connect gate="-DRQ1" pin="P" pad="B18"/>
<connect gate="-DRQ2" pin="P" pad="B6"/>
<connect gate="-DRQ3" pin="P" pad="B16"/>
<connect gate="-DRQ5" pin="P" pad="D11"/>
<connect gate="-DRQ6" pin="P" pad="D13"/>
<connect gate="-DRQ7" pin="P" pad="D15"/>
<connect gate="-EX16" pin="P" pad="E7"/>
<connect gate="-EX32" pin="P" pad="E4"/>
<connect gate="-EXRDY" pin="P" pad="E3"/>
<connect gate="-IO16" pin="P" pad="D2"/>
<connect gate="-IORC" pin="P" pad="B14"/>
<connect gate="-IOWC" pin="P" pad="B13"/>
<connect gate="-IRQ10" pin="P" pad="D3"/>
<connect gate="-IRQ11" pin="P" pad="D4"/>
<connect gate="-IRQ12" pin="P" pad="D5"/>
<connect gate="-IRQ13" pin="P" pad="D6"/>
<connect gate="-IRQ14" pin="P" pad="D7"/>
<connect gate="-IRQ2" pin="P" pad="B4"/>
<connect gate="-IRQ3" pin="P" pad="B25"/>
<connect gate="-IRQ4" pin="P" pad="B24"/>
<connect gate="-IRQ5" pin="P" pad="B23"/>
<connect gate="-IRQ6" pin="P" pad="B22"/>
<connect gate="-IRQ7" pin="P" pad="B21"/>
<connect gate="-LA10" pin="P" pad="F31"/>
<connect gate="-LA11" pin="P" pad="E29"/>
<connect gate="-LA12" pin="P" pad="E28"/>
<connect gate="-LA13" pin="P" pad="E27"/>
<connect gate="-LA14" pin="P" pad="F27"/>
<connect gate="-LA15" pin="P" pad="E26"/>
<connect gate="-LA16" pin="P" pad="F26"/>
<connect gate="-LA17" pin="P" pad="C8"/>
<connect gate="-LA18" pin="P" pad="C7"/>
<connect gate="-LA19" pin="P" pad="C6"/>
<connect gate="-LA2" pin="P" pad="H5"/>
<connect gate="-LA20" pin="P" pad="C5"/>
<connect gate="-LA21" pin="P" pad="C4"/>
<connect gate="-LA22" pin="P" pad="C3"/>
<connect gate="-LA23" pin="P" pad="C2"/>
<connect gate="-LA24" pin="P" pad="F24"/>
<connect gate="-LA25" pin="P" pad="E23"/>
<connect gate="-LA26" pin="P" pad="F23"/>
<connect gate="-LA27" pin="P" pad="E22"/>
<connect gate="-LA28" pin="P" pad="E21"/>
<connect gate="-LA29" pin="P" pad="F21"/>
<connect gate="-LA3" pin="P" pad="G4"/>
<connect gate="-LA30" pin="P" pad="E20"/>
<connect gate="-LA31" pin="P" pad="E18"/>
<connect gate="-LA4" pin="P" pad="G3"/>
<connect gate="-LA5" pin="P" pad="H3"/>
<connect gate="-LA6" pin="P" pad="H2"/>
<connect gate="-LA7" pin="P" pad="G1"/>
<connect gate="-LA8" pin="P" pad="H1"/>
<connect gate="-LA9" pin="P" pad="E31"/>
<connect gate="-LOCK" pin="P" pad="F11"/>
<connect gate="-M/IO" pin="P" pad="F10"/>
<connect gate="-M16" pin="P" pad="D1"/>
<connect gate="-MAKX" pin="P" pad="H19"/>
<connect gate="-MRDC" pin="P" pad="C9"/>
<connect gate="-MREQX" pin="P" pad="G19"/>
<connect gate="-MSBURST" pin="P" pad="E9"/>
<connect gate="-MWTC" pin="P" pad="C10"/>
<connect gate="-NOWS" pin="P" pad="B8"/>
<connect gate="-OSC" pin="P" pad="B30"/>
<connect gate="-REFRESH" pin="P" pad="B19"/>
<connect gate="-RESERV1" pin="RSV" pad="E12"/>
<connect gate="-RESERV2" pin="RSV" pad="E13"/>
<connect gate="-RESERV3" pin="RSV" pad="E14"/>
<connect gate="-RESERV4" pin="RSV" pad="F4"/>
<connect gate="-RESERV5" pin="RSV" pad="F5"/>
<connect gate="-RESERV6" pin="RSV" pad="F7"/>
<connect gate="-RESERV7" pin="RSV" pad="F8"/>
<connect gate="-RESERV8" pin="RSV" pad="F12"/>
<connect gate="-RESERV9" pin="RSV" pad="F14"/>
<connect gate="-RESV10" pin="P" pad="B2"/>
<connect gate="-SA0" pin="P" pad="A31"/>
<connect gate="-SA1" pin="P" pad="A30"/>
<connect gate="-SA10" pin="P" pad="A21"/>
<connect gate="-SA11" pin="P" pad="A20"/>
<connect gate="-SA12" pin="P" pad="A19"/>
<connect gate="-SA13" pin="P" pad="A18"/>
<connect gate="-SA14" pin="P" pad="A17"/>
<connect gate="-SA15" pin="P" pad="A16"/>
<connect gate="-SA16" pin="P" pad="A15"/>
<connect gate="-SA17" pin="P" pad="A14"/>
<connect gate="-SA18" pin="P" pad="A13"/>
<connect gate="-SA19" pin="P" pad="A12"/>
<connect gate="-SA2" pin="P" pad="A29"/>
<connect gate="-SA3" pin="P" pad="A28"/>
<connect gate="-SA4" pin="P" pad="A27"/>
<connect gate="-SA5" pin="P" pad="A26"/>
<connect gate="-SA6" pin="P" pad="A25"/>
<connect gate="-SA7" pin="P" pad="A24"/>
<connect gate="-SA8" pin="P" pad="A23"/>
<connect gate="-SA9" pin="P" pad="A22"/>
<connect gate="-SBHE" pin="P" pad="C1"/>
<connect gate="-SD0" pin="P" pad="A9"/>
<connect gate="-SD1" pin="P" pad="A8"/>
<connect gate="-SD10" pin="P" pad="C13"/>
<connect gate="-SD11" pin="P" pad="C14"/>
<connect gate="-SD12" pin="P" pad="C15"/>
<connect gate="-SD13" pin="P" pad="C16"/>
<connect gate="-SD14" pin="P" pad="C17"/>
<connect gate="-SD15" pin="P" pad="C18"/>
<connect gate="-SD16" pin="P" pad="H7"/>
<connect gate="-SD17" pin="P" pad="G7"/>
<connect gate="-SD18" pin="P" pad="H8"/>
<connect gate="-SD19" pin="P" pad="G8"/>
<connect gate="-SD2" pin="P" pad="A7"/>
<connect gate="-SD20" pin="P" pad="G9"/>
<connect gate="-SD21" pin="P" pad="H10"/>
<connect gate="-SD22" pin="P" pad="G10"/>
<connect gate="-SD23" pin="P" pad="H11"/>
<connect gate="-SD24" pin="P" pad="H12"/>
<connect gate="-SD25" pin="P" pad="G12"/>
<connect gate="-SD26" pin="P" pad="G13"/>
<connect gate="-SD27" pin="P" pad="H14"/>
<connect gate="-SD28" pin="P" pad="G14"/>
<connect gate="-SD29" pin="P" pad="H16"/>
<connect gate="-SD3" pin="P" pad="A6"/>
<connect gate="-SD30" pin="P" pad="G17"/>
<connect gate="-SD31" pin="P" pad="G18"/>
<connect gate="-SD4" pin="P" pad="A5"/>
<connect gate="-SD5" pin="P" pad="A4"/>
<connect gate="-SD6" pin="P" pad="A3"/>
<connect gate="-SD7" pin="P" pad="A2"/>
<connect gate="-SD8" pin="P" pad="C11"/>
<connect gate="-SD9" pin="P" pad="C12"/>
<connect gate="-SLBURST" pin="P" pad="E8"/>
<connect gate="-SMRDC" pin="P" pad="B12"/>
<connect gate="-SMWTC" pin="P" pad="B11"/>
<connect gate="-START" pin="P" pad="E2"/>
<connect gate="-TC" pin="P" pad="B27"/>
<connect gate="-W/R" pin="P" pad="E10"/>
<connect gate="GND0" pin="GND" pad="E5"/>
<connect gate="GND1" pin="GND" pad="E11"/>
<connect gate="GND10" pin="GND" pad="F30"/>
<connect gate="GND11" pin="GND" pad="B1"/>
<connect gate="GND12" pin="GND" pad="B10"/>
<connect gate="GND13" pin="GND" pad="B31"/>
<connect gate="GND14" pin="GND" pad="G2"/>
<connect gate="GND15" pin="GND" pad="G5"/>
<connect gate="GND16" pin="GND" pad="G11"/>
<connect gate="GND17" pin="GND" pad="G16"/>
<connect gate="GND18" pin="GND" pad="H9"/>
<connect gate="GND19" pin="GND" pad="H13"/>
<connect gate="GND2" pin="GND" pad="E15"/>
<connect gate="GND20" pin="GND" pad="D18"/>
<connect gate="GND3" pin="GND" pad="E19"/>
<connect gate="GND4" pin="GND" pad="E24"/>
<connect gate="GND5" pin="GND" pad="E30"/>
<connect gate="GND6" pin="GND" pad="F1"/>
<connect gate="GND7" pin="GND" pad="F13"/>
<connect gate="GND8" pin="GND" pad="F19"/>
<connect gate="GND9" pin="GND" pad="F22"/>
<connect gate="MASTER16" pin="P" pad="D17"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SC242" prefix="X" uservalue="yes">
<description>&lt;B&gt;SLOT1 CONNECTOR&lt;/B&gt;&lt;p&gt;
Intel</description>
<gates>
<gate name="A1" symbol="FEMRVAL"/>
<gate name="A2" symbol="FEMREC"/>
<gate name="A3" symbol="FEMREC"/>
<gate name="A4" symbol="FEMREC"/>
<gate name="A5" symbol="FEMREC"/>
<gate name="A6" symbol="FEMREC"/>
<gate name="A7" symbol="FEMREC"/>
<gate name="A8" symbol="FEMREC"/>
<gate name="A9" symbol="FEMREC"/>
<gate name="A10" symbol="FEMREC"/>
<gate name="A11" symbol="FEMREC"/>
<gate name="A12" symbol="FEMREC"/>
<gate name="A13" symbol="FEMREC"/>
<gate name="A14" symbol="FEMREC"/>
<gate name="A15" symbol="FEMREC"/>
<gate name="A16" symbol="FEMREC"/>
<gate name="A17" symbol="FEMREC"/>
<gate name="A18" symbol="FEMREC"/>
<gate name="A19" symbol="FEMREC"/>
<gate name="A20" symbol="FEMREC"/>
<gate name="A21" symbol="FEMREC"/>
<gate name="A22" symbol="FEMREC"/>
<gate name="A23" symbol="FEMREC"/>
<gate name="A24" symbol="FEMREC"/>
<gate name="A25" symbol="FEMREC"/>
<gate name="A26" symbol="FEMREC"/>
<gate name="A27" symbol="FEMREC"/>
<gate name="A28" symbol="FEMREC"/>
<gate name="A29" symbol="FEMREC"/>
<gate name="A30" symbol="FEMREC"/>
<gate name="A31" symbol="FEMREC"/>
<gate name="A32" symbol="FEMREC"/>
<gate name="A33" symbol="FEMREC"/>
<gate name="A34" symbol="FEMREC"/>
<gate name="A35" symbol="FEMREC"/>
<gate name="A36" symbol="FEMREC"/>
<gate name="A37" symbol="FEMREC"/>
<gate name="A38" symbol="FEMREC"/>
<gate name="A39" symbol="FEMREC"/>
<gate name="A40" symbol="FEMREC"/>
<gate name="A41" symbol="FEMREC"/>
<gate name="A42" symbol="FEMREC"/>
<gate name="A43" symbol="FEMREC"/>
<gate name="A44" symbol="FEMREC"/>
<gate name="A45" symbol="FEMREC"/>
<gate name="A46" symbol="FEMREC"/>
<gate name="A47" symbol="FEMREC"/>
<gate name="A48" symbol="FEMREC"/>
<gate name="A49" symbol="FEMREC"/>
<gate name="A50" symbol="FEMREC"/>
<gate name="A51" symbol="FEMREC"/>
<gate name="A52" symbol="FEMREC"/>
<gate name="A53" symbol="FEMREC"/>
<gate name="A54" symbol="FEMREC"/>
<gate name="A55" symbol="FEMREC"/>
<gate name="A56" symbol="FEMREC"/>
<gate name="A57" symbol="FEMREC"/>
<gate name="A58" symbol="FEMREC"/>
<gate name="A59" symbol="FEMREC"/>
<gate name="A60" symbol="FEMREC"/>
<gate name="A61" symbol="FEMREC"/>
<gate name="A62" symbol="FEMREC"/>
<gate name="A63" symbol="FEMREC"/>
<gate name="A64" symbol="FEMREC"/>
<gate name="A65" symbol="FEMREC"/>
<gate name="A66" symbol="FEMREC"/>
<gate name="A67" symbol="FEMREC"/>
<gate name="A68" symbol="FEMREC"/>
<gate name="A69" symbol="FEMREC"/>
<gate name="A70" symbol="FEMREC"/>
<gate name="A71" symbol="FEMREC"/>
<gate name="A72" symbol="FEMREC"/>
<gate name="A73" symbol="FEMREC"/>
<gate name="A74" symbol="FEMREC"/>
<gate name="A75" symbol="FEMREC"/>
<gate name="A76" symbol="FEMREC"/>
<gate name="A77" symbol="FEMREC"/>
<gate name="A78" symbol="FEMREC"/>
<gate name="A79" symbol="FEMREC"/>
<gate name="A80" symbol="FEMREC"/>
<gate name="A81" symbol="FEMREC"/>
<gate name="A82" symbol="FEMREC"/>
<gate name="A83" symbol="FEMREC"/>
<gate name="A84" symbol="FEMREC"/>
<gate name="A85" symbol="FEMREC"/>
<gate name="A86" symbol="FEMREC"/>
<gate name="A87" symbol="FEMREC"/>
<gate name="A88" symbol="FEMREC"/>
<gate name="A89" symbol="FEMREC"/>
<gate name="A90" symbol="FEMREC"/>
<gate name="A91" symbol="FEMREC"/>
<gate name="A92" symbol="FEMREC"/>
<gate name="A93" symbol="FEMREC"/>
<gate name="A94" symbol="FEMREC"/>
<gate name="A95" symbol="FEMREC"/>
<gate name="A96" symbol="FEMREC"/>
<gate name="A97" symbol="FEMREC"/>
<gate name="A98" symbol="FEMREC"/>
<gate name="A99" symbol="FEMREC"/>
<gate name="A100" symbol="FEMREC"/>
<gate name="A101" symbol="FEMREC"/>
<gate name="A102" symbol="FEMREC"/>
<gate name="A103" symbol="FEMREC"/>
<gate name="A104" symbol="FEMREC"/>
<gate name="A105" symbol="FEMREC"/>
<gate name="A106" symbol="FEMREC"/>
<gate name="A107" symbol="FEMREC"/>
<gate name="A108" symbol="FEMREC"/>
<gate name="A109" symbol="FEMREC"/>
<gate name="A110" symbol="FEMREC"/>
<gate name="A111" symbol="FEMREC"/>
<gate name="A112" symbol="FEMREC"/>
<gate name="A113" symbol="FEMREC"/>
<gate name="A114" symbol="FEMREC"/>
<gate name="A115" symbol="FEMREC"/>
<gate name="A116" symbol="FEMREC"/>
<gate name="A117" symbol="FEMREC"/>
<gate name="A118" symbol="FEMREC"/>
<gate name="A119" symbol="FEMREC"/>
<gate name="A120" symbol="FEMREC"/>
<gate name="A121" symbol="FEMREC"/>
<gate name="B1" symbol="FEMRVAL"/>
<gate name="B2" symbol="FEMREC"/>
<gate name="B3" symbol="FEMREC"/>
<gate name="B4" symbol="FEMREC"/>
<gate name="B5" symbol="FEMREC"/>
<gate name="B6" symbol="FEMREC"/>
<gate name="B7" symbol="FEMREC"/>
<gate name="B8" symbol="FEMREC"/>
<gate name="B9" symbol="FEMREC"/>
<gate name="B10" symbol="FEMREC"/>
<gate name="B11" symbol="FEMREC"/>
<gate name="B12" symbol="FEMREC"/>
<gate name="B13" symbol="FEMREC"/>
<gate name="B14" symbol="FEMREC"/>
<gate name="B15" symbol="FEMREC"/>
<gate name="B16" symbol="FEMREC"/>
<gate name="B17" symbol="FEMREC"/>
<gate name="B18" symbol="FEMREC"/>
<gate name="B19" symbol="FEMREC"/>
<gate name="B20" symbol="FEMREC"/>
<gate name="B21" symbol="FEMREC"/>
<gate name="B22" symbol="FEMREC"/>
<gate name="B23" symbol="FEMREC"/>
<gate name="B24" symbol="FEMREC"/>
<gate name="B25" symbol="FEMREC"/>
<gate name="B26" symbol="FEMREC"/>
<gate name="B27" symbol="FEMREC"/>
<gate name="B28" symbol="FEMREC"/>
<gate name="B29" symbol="FEMREC"/>
<gate name="B30" symbol="FEMREC"/>
<gate name="B31" symbol="FEMREC"/>
<gate name="B32" symbol="FEMREC"/>
<gate name="B33" symbol="FEMREC"/>
<gate name="B34" symbol="FEMREC"/>
<gate name="B35" symbol="FEMREC"/>
<gate name="B36" symbol="FEMREC"/>
<gate name="B37" symbol="FEMREC"/>
<gate name="B38" symbol="FEMREC"/>
<gate name="B39" symbol="FEMREC"/>
<gate name="B40" symbol="FEMREC"/>
<gate name="B41" symbol="FEMREC"/>
<gate name="B42" symbol="FEMREC"/>
<gate name="B43" symbol="FEMREC"/>
<gate name="B44" symbol="FEMREC"/>
<gate name="B45" symbol="FEMREC"/>
<gate name="B46" symbol="FEMREC"/>
<gate name="B47" symbol="FEMREC"/>
<gate name="B48" symbol="FEMREC"/>
<gate name="B49" symbol="FEMREC"/>
<gate name="B50" symbol="FEMREC"/>
<gate name="B51" symbol="FEMREC"/>
<gate name="B52" symbol="FEMREC"/>
<gate name="B53" symbol="FEMREC"/>
<gate name="B54" symbol="FEMREC"/>
<gate name="B55" symbol="FEMREC"/>
<gate name="B56" symbol="FEMREC"/>
<gate name="B57" symbol="FEMREC"/>
<gate name="B58" symbol="FEMREC"/>
<gate name="B59" symbol="FEMREC"/>
<gate name="B60" symbol="FEMREC"/>
<gate name="B61" symbol="FEMREC"/>
<gate name="B62" symbol="FEMREC"/>
<gate name="B63" symbol="FEMREC"/>
<gate name="B64" symbol="FEMREC"/>
<gate name="B65" symbol="FEMREC"/>
<gate name="B66" symbol="FEMREC"/>
<gate name="B67" symbol="FEMREC"/>
<gate name="B68" symbol="FEMREC"/>
<gate name="B69" symbol="FEMREC"/>
<gate name="B70" symbol="FEMREC"/>
<gate name="B71" symbol="FEMREC"/>
<gate name="B72" symbol="FEMREC"/>
<gate name="B73" symbol="FEMREC"/>
<gate name="B74" symbol="FEMREC"/>
<gate name="B75" symbol="FEMREC"/>
<gate name="B76" symbol="FEMREC"/>
<gate name="B77" symbol="FEMREC"/>
<gate name="B78" symbol="FEMREC"/>
<gate name="B79" symbol="FEMREC"/>
<gate name="B80" symbol="FEMREC"/>
<gate name="B81" symbol="FEMREC"/>
<gate name="B82" symbol="FEMREC"/>
<gate name="B83" symbol="FEMREC"/>
<gate name="B84" symbol="FEMREC"/>
<gate name="B85" symbol="FEMREC"/>
<gate name="B86" symbol="FEMREC"/>
<gate name="B87" symbol="FEMREC"/>
<gate name="B88" symbol="FEMREC"/>
<gate name="B89" symbol="FEMREC"/>
<gate name="B90" symbol="FEMREC"/>
<gate name="B91" symbol="FEMREC"/>
<gate name="B92" symbol="FEMREC"/>
<gate name="B93" symbol="FEMREC"/>
<gate name="B94" symbol="FEMREC"/>
<gate name="B95" symbol="FEMREC"/>
<gate name="B96" symbol="FEMREC"/>
<gate name="B97" symbol="FEMREC"/>
<gate name="B98" symbol="FEMREC"/>
<gate name="B99" symbol="FEMREC"/>
<gate name="B100" symbol="FEMREC"/>
<gate name="B101" symbol="FEMREC"/>
<gate name="B102" symbol="FEMREC"/>
<gate name="B103" symbol="FEMREC"/>
<gate name="B104" symbol="FEMREC"/>
<gate name="B105" symbol="FEMREC"/>
<gate name="B106" symbol="FEMREC"/>
<gate name="B107" symbol="FEMREC"/>
<gate name="B108" symbol="FEMREC"/>
<gate name="B109" symbol="FEMREC"/>
<gate name="B110" symbol="FEMREC"/>
<gate name="B111" symbol="FEMREC"/>
<gate name="B112" symbol="FEMREC"/>
<gate name="B113" symbol="FEMREC"/>
<gate name="B114" symbol="FEMREC"/>
<gate name="B115" symbol="FEMREC"/>
<gate name="B116" symbol="FEMREC"/>
<gate name="B117" symbol="FEMREC"/>
<gate name="B118" symbol="FEMREC"/>
<gate name="B119" symbol="FEMREC"/>
<gate name="B120" symbol="FEMREC"/>
<gate name="B121" symbol="FEMREC"/>
</gates>
<devices>
<device name="" package="SC242CON">
<connects>
<connect gate="A1" pin="P" pad="A1"/>
<connect gate="A10" pin="P" pad="A10"/>
<connect gate="A100" pin="P" pad="A100"/>
<connect gate="A101" pin="P" pad="A101"/>
<connect gate="A102" pin="P" pad="A102"/>
<connect gate="A103" pin="P" pad="A103"/>
<connect gate="A104" pin="P" pad="A104"/>
<connect gate="A105" pin="P" pad="A105"/>
<connect gate="A106" pin="P" pad="A106"/>
<connect gate="A107" pin="P" pad="A107"/>
<connect gate="A108" pin="P" pad="A108"/>
<connect gate="A109" pin="P" pad="A109"/>
<connect gate="A11" pin="P" pad="A11"/>
<connect gate="A110" pin="P" pad="A110"/>
<connect gate="A111" pin="P" pad="A111"/>
<connect gate="A112" pin="P" pad="A112"/>
<connect gate="A113" pin="P" pad="A113"/>
<connect gate="A114" pin="P" pad="A114"/>
<connect gate="A115" pin="P" pad="A115"/>
<connect gate="A116" pin="P" pad="A116"/>
<connect gate="A117" pin="P" pad="A117"/>
<connect gate="A118" pin="P" pad="A118"/>
<connect gate="A119" pin="P" pad="A119"/>
<connect gate="A12" pin="P" pad="A12"/>
<connect gate="A120" pin="P" pad="A120"/>
<connect gate="A121" pin="P" pad="A121"/>
<connect gate="A13" pin="P" pad="A13"/>
<connect gate="A14" pin="P" pad="A14"/>
<connect gate="A15" pin="P" pad="A15"/>
<connect gate="A16" pin="P" pad="A16"/>
<connect gate="A17" pin="P" pad="A17"/>
<connect gate="A18" pin="P" pad="A18"/>
<connect gate="A19" pin="P" pad="A19"/>
<connect gate="A2" pin="P" pad="A2"/>
<connect gate="A20" pin="P" pad="A20"/>
<connect gate="A21" pin="P" pad="A21"/>
<connect gate="A22" pin="P" pad="A22"/>
<connect gate="A23" pin="P" pad="A23"/>
<connect gate="A24" pin="P" pad="A24"/>
<connect gate="A25" pin="P" pad="A25"/>
<connect gate="A26" pin="P" pad="A26"/>
<connect gate="A27" pin="P" pad="A27"/>
<connect gate="A28" pin="P" pad="A28"/>
<connect gate="A29" pin="P" pad="A29"/>
<connect gate="A3" pin="P" pad="A3"/>
<connect gate="A30" pin="P" pad="A30"/>
<connect gate="A31" pin="P" pad="A31"/>
<connect gate="A32" pin="P" pad="A32"/>
<connect gate="A33" pin="P" pad="A33"/>
<connect gate="A34" pin="P" pad="A34"/>
<connect gate="A35" pin="P" pad="A35"/>
<connect gate="A36" pin="P" pad="A36"/>
<connect gate="A37" pin="P" pad="A37"/>
<connect gate="A38" pin="P" pad="A38"/>
<connect gate="A39" pin="P" pad="A39"/>
<connect gate="A4" pin="P" pad="A4"/>
<connect gate="A40" pin="P" pad="A40"/>
<connect gate="A41" pin="P" pad="A41"/>
<connect gate="A42" pin="P" pad="A42"/>
<connect gate="A43" pin="P" pad="A43"/>
<connect gate="A44" pin="P" pad="A44"/>
<connect gate="A45" pin="P" pad="A45"/>
<connect gate="A46" pin="P" pad="A46"/>
<connect gate="A47" pin="P" pad="A47"/>
<connect gate="A48" pin="P" pad="A48"/>
<connect gate="A49" pin="P" pad="A49"/>
<connect gate="A5" pin="P" pad="A5"/>
<connect gate="A50" pin="P" pad="A50"/>
<connect gate="A51" pin="P" pad="A51"/>
<connect gate="A52" pin="P" pad="A52"/>
<connect gate="A53" pin="P" pad="A53"/>
<connect gate="A54" pin="P" pad="A54"/>
<connect gate="A55" pin="P" pad="A55"/>
<connect gate="A56" pin="P" pad="A56"/>
<connect gate="A57" pin="P" pad="A57"/>
<connect gate="A58" pin="P" pad="A58"/>
<connect gate="A59" pin="P" pad="A59"/>
<connect gate="A6" pin="P" pad="A6"/>
<connect gate="A60" pin="P" pad="A60"/>
<connect gate="A61" pin="P" pad="A61"/>
<connect gate="A62" pin="P" pad="A62"/>
<connect gate="A63" pin="P" pad="A63"/>
<connect gate="A64" pin="P" pad="A64"/>
<connect gate="A65" pin="P" pad="A65"/>
<connect gate="A66" pin="P" pad="A66"/>
<connect gate="A67" pin="P" pad="A67"/>
<connect gate="A68" pin="P" pad="A68"/>
<connect gate="A69" pin="P" pad="A69"/>
<connect gate="A7" pin="P" pad="A7"/>
<connect gate="A70" pin="P" pad="A70"/>
<connect gate="A71" pin="P" pad="A71"/>
<connect gate="A72" pin="P" pad="A72"/>
<connect gate="A73" pin="P" pad="A73"/>
<connect gate="A74" pin="P" pad="A74"/>
<connect gate="A75" pin="P" pad="A75"/>
<connect gate="A76" pin="P" pad="A76"/>
<connect gate="A77" pin="P" pad="A77"/>
<connect gate="A78" pin="P" pad="A78"/>
<connect gate="A79" pin="P" pad="A79"/>
<connect gate="A8" pin="P" pad="A8"/>
<connect gate="A80" pin="P" pad="A80"/>
<connect gate="A81" pin="P" pad="A81"/>
<connect gate="A82" pin="P" pad="A82"/>
<connect gate="A83" pin="P" pad="A83"/>
<connect gate="A84" pin="P" pad="A84"/>
<connect gate="A85" pin="P" pad="A85"/>
<connect gate="A86" pin="P" pad="A86"/>
<connect gate="A87" pin="P" pad="A87"/>
<connect gate="A88" pin="P" pad="A88"/>
<connect gate="A89" pin="P" pad="A89"/>
<connect gate="A9" pin="P" pad="A9"/>
<connect gate="A90" pin="P" pad="A90"/>
<connect gate="A91" pin="P" pad="A91"/>
<connect gate="A92" pin="P" pad="A92"/>
<connect gate="A93" pin="P" pad="A93"/>
<connect gate="A94" pin="P" pad="A94"/>
<connect gate="A95" pin="P" pad="A95"/>
<connect gate="A96" pin="P" pad="A96"/>
<connect gate="A97" pin="P" pad="A97"/>
<connect gate="A98" pin="P" pad="A98"/>
<connect gate="A99" pin="P" pad="A99"/>
<connect gate="B1" pin="P" pad="B1"/>
<connect gate="B10" pin="P" pad="B10"/>
<connect gate="B100" pin="P" pad="B100"/>
<connect gate="B101" pin="P" pad="B101"/>
<connect gate="B102" pin="P" pad="B102"/>
<connect gate="B103" pin="P" pad="B103"/>
<connect gate="B104" pin="P" pad="B104"/>
<connect gate="B105" pin="P" pad="B105"/>
<connect gate="B106" pin="P" pad="B106"/>
<connect gate="B107" pin="P" pad="B107"/>
<connect gate="B108" pin="P" pad="B108"/>
<connect gate="B109" pin="P" pad="B109"/>
<connect gate="B11" pin="P" pad="B11"/>
<connect gate="B110" pin="P" pad="B110"/>
<connect gate="B111" pin="P" pad="B111"/>
<connect gate="B112" pin="P" pad="B112"/>
<connect gate="B113" pin="P" pad="B113"/>
<connect gate="B114" pin="P" pad="B114"/>
<connect gate="B115" pin="P" pad="B115"/>
<connect gate="B116" pin="P" pad="B116"/>
<connect gate="B117" pin="P" pad="B117"/>
<connect gate="B118" pin="P" pad="B118"/>
<connect gate="B119" pin="P" pad="B119"/>
<connect gate="B12" pin="P" pad="B12"/>
<connect gate="B120" pin="P" pad="B120"/>
<connect gate="B121" pin="P" pad="B121"/>
<connect gate="B13" pin="P" pad="B13"/>
<connect gate="B14" pin="P" pad="B14"/>
<connect gate="B15" pin="P" pad="B15"/>
<connect gate="B16" pin="P" pad="B16"/>
<connect gate="B17" pin="P" pad="B17"/>
<connect gate="B18" pin="P" pad="B18"/>
<connect gate="B19" pin="P" pad="B19"/>
<connect gate="B2" pin="P" pad="B2"/>
<connect gate="B20" pin="P" pad="B20"/>
<connect gate="B21" pin="P" pad="B21"/>
<connect gate="B22" pin="P" pad="B22"/>
<connect gate="B23" pin="P" pad="B23"/>
<connect gate="B24" pin="P" pad="B24"/>
<connect gate="B25" pin="P" pad="B25"/>
<connect gate="B26" pin="P" pad="B26"/>
<connect gate="B27" pin="P" pad="B27"/>
<connect gate="B28" pin="P" pad="B28"/>
<connect gate="B29" pin="P" pad="B29"/>
<connect gate="B3" pin="P" pad="B3"/>
<connect gate="B30" pin="P" pad="B30"/>
<connect gate="B31" pin="P" pad="B31"/>
<connect gate="B32" pin="P" pad="B32"/>
<connect gate="B33" pin="P" pad="B33"/>
<connect gate="B34" pin="P" pad="B34"/>
<connect gate="B35" pin="P" pad="B35"/>
<connect gate="B36" pin="P" pad="B36"/>
<connect gate="B37" pin="P" pad="B37"/>
<connect gate="B38" pin="P" pad="B38"/>
<connect gate="B39" pin="P" pad="B39"/>
<connect gate="B4" pin="P" pad="B4"/>
<connect gate="B40" pin="P" pad="B40"/>
<connect gate="B41" pin="P" pad="B41"/>
<connect gate="B42" pin="P" pad="B42"/>
<connect gate="B43" pin="P" pad="B43"/>
<connect gate="B44" pin="P" pad="B44"/>
<connect gate="B45" pin="P" pad="B45"/>
<connect gate="B46" pin="P" pad="B46"/>
<connect gate="B47" pin="P" pad="B47"/>
<connect gate="B48" pin="P" pad="B48"/>
<connect gate="B49" pin="P" pad="B49"/>
<connect gate="B5" pin="P" pad="B5"/>
<connect gate="B50" pin="P" pad="B50"/>
<connect gate="B51" pin="P" pad="B51"/>
<connect gate="B52" pin="P" pad="B52"/>
<connect gate="B53" pin="P" pad="B53"/>
<connect gate="B54" pin="P" pad="B54"/>
<connect gate="B55" pin="P" pad="B55"/>
<connect gate="B56" pin="P" pad="B56"/>
<connect gate="B57" pin="P" pad="B57"/>
<connect gate="B58" pin="P" pad="B58"/>
<connect gate="B59" pin="P" pad="B59"/>
<connect gate="B6" pin="P" pad="B6"/>
<connect gate="B60" pin="P" pad="B60"/>
<connect gate="B61" pin="P" pad="B61"/>
<connect gate="B62" pin="P" pad="B62"/>
<connect gate="B63" pin="P" pad="B63"/>
<connect gate="B64" pin="P" pad="B64"/>
<connect gate="B65" pin="P" pad="B65"/>
<connect gate="B66" pin="P" pad="B66"/>
<connect gate="B67" pin="P" pad="B67"/>
<connect gate="B68" pin="P" pad="B68"/>
<connect gate="B69" pin="P" pad="B69"/>
<connect gate="B7" pin="P" pad="B7"/>
<connect gate="B70" pin="P" pad="B70"/>
<connect gate="B71" pin="P" pad="B71"/>
<connect gate="B72" pin="P" pad="B72"/>
<connect gate="B73" pin="P" pad="B73"/>
<connect gate="B74" pin="P" pad="B74"/>
<connect gate="B75" pin="P" pad="B75"/>
<connect gate="B76" pin="P" pad="B76"/>
<connect gate="B77" pin="P" pad="B77"/>
<connect gate="B78" pin="P" pad="B78"/>
<connect gate="B79" pin="P" pad="B79"/>
<connect gate="B8" pin="P" pad="B8"/>
<connect gate="B80" pin="P" pad="B80"/>
<connect gate="B81" pin="P" pad="B81"/>
<connect gate="B82" pin="P" pad="B82"/>
<connect gate="B83" pin="P" pad="B83"/>
<connect gate="B84" pin="P" pad="B84"/>
<connect gate="B85" pin="P" pad="B85"/>
<connect gate="B86" pin="P" pad="B86"/>
<connect gate="B87" pin="P" pad="B87"/>
<connect gate="B88" pin="P" pad="B88"/>
<connect gate="B89" pin="P" pad="B89"/>
<connect gate="B9" pin="P" pad="B9"/>
<connect gate="B90" pin="P" pad="B90"/>
<connect gate="B91" pin="P" pad="B91"/>
<connect gate="B92" pin="P" pad="B92"/>
<connect gate="B93" pin="P" pad="B93"/>
<connect gate="B94" pin="P" pad="B94"/>
<connect gate="B95" pin="P" pad="B95"/>
<connect gate="B96" pin="P" pad="B96"/>
<connect gate="B97" pin="P" pad="B97"/>
<connect gate="B98" pin="P" pad="B98"/>
<connect gate="B99" pin="P" pad="B99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AGP" prefix="X">
<description>&lt;b&gt;AGP Slot&lt;/b&gt; AMP connctor 145263 &amp;gt;PCT-GF40&amp;lt;&lt;p&gt;
124 Position 1mm, card edge connector&lt;br&gt;
Drawing No: C-145263&lt;br&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_145263_H.pdf</description>
<gates>
<gate name="-1" symbol="FEMRVAL"/>
<gate name="-2" symbol="FEMRVAL"/>
<gate name="-3" symbol="FEMREC"/>
<gate name="-4" symbol="FEMREC"/>
<gate name="-5" symbol="FEMREC"/>
<gate name="-6" symbol="FEMREC"/>
<gate name="-7" symbol="FEMREC"/>
<gate name="-8" symbol="FEMREC"/>
<gate name="-9" symbol="FEMREC"/>
<gate name="-10" symbol="FEMREC"/>
<gate name="-11" symbol="FEMREC"/>
<gate name="-12" symbol="FEMREC"/>
<gate name="-13" symbol="FEMREC"/>
<gate name="-14" symbol="FEMREC"/>
<gate name="-15" symbol="FEMREC"/>
<gate name="-16" symbol="FEMREC"/>
<gate name="-17" symbol="FEMREC"/>
<gate name="-18" symbol="FEMREC"/>
<gate name="-19" symbol="FEMREC"/>
<gate name="-20" symbol="FEMREC"/>
<gate name="-21" symbol="FEMREC"/>
<gate name="-22" symbol="FEMREC"/>
<gate name="-23" symbol="FEMREC"/>
<gate name="-24" symbol="FEMREC"/>
<gate name="-25" symbol="FEMREC"/>
<gate name="-26" symbol="FEMREC"/>
<gate name="-27" symbol="FEMREC"/>
<gate name="-28" symbol="FEMREC"/>
<gate name="-29" symbol="FEMREC"/>
<gate name="-30" symbol="FEMREC"/>
<gate name="-31" symbol="FEMREC"/>
<gate name="-32" symbol="FEMREC"/>
<gate name="-33" symbol="FEMREC"/>
<gate name="-34" symbol="FEMREC"/>
<gate name="-35" symbol="FEMREC"/>
<gate name="-36" symbol="FEMREC"/>
<gate name="-37" symbol="FEMREC"/>
<gate name="-38" symbol="FEMREC"/>
<gate name="-39" symbol="FEMREC"/>
<gate name="-40" symbol="FEMREC"/>
<gate name="-41" symbol="FEMREC"/>
<gate name="-42" symbol="FEMREC"/>
<gate name="-43" symbol="FEMREC"/>
<gate name="-44" symbol="FEMREC"/>
<gate name="-45" symbol="FEMREC"/>
<gate name="-46" symbol="FEMREC"/>
<gate name="-47" symbol="FEMREC"/>
<gate name="-48" symbol="FEMREC"/>
<gate name="-49" symbol="FEMREC"/>
<gate name="-50" symbol="FEMREC"/>
<gate name="-51" symbol="FEMREC"/>
<gate name="-52" symbol="FEMREC"/>
<gate name="-53" symbol="FEMREC"/>
<gate name="-54" symbol="FEMREC"/>
<gate name="-55" symbol="FEMREC"/>
<gate name="-56" symbol="FEMREC"/>
<gate name="-57" symbol="FEMREC"/>
<gate name="-58" symbol="FEMREC"/>
<gate name="-59" symbol="FEMREC"/>
<gate name="-60" symbol="FEMREC"/>
<gate name="-61" symbol="FEMREC"/>
<gate name="-62" symbol="FEMREC"/>
<gate name="-63" symbol="FEMREC"/>
<gate name="-64" symbol="FEMREC"/>
<gate name="-65" symbol="FEMREC"/>
<gate name="-66" symbol="FEMREC"/>
<gate name="-67" symbol="FEMREC"/>
<gate name="-68" symbol="FEMREC"/>
<gate name="-69" symbol="FEMREC"/>
<gate name="-70" symbol="FEMREC"/>
<gate name="-71" symbol="FEMREC"/>
<gate name="-72" symbol="FEMREC"/>
<gate name="-73" symbol="FEMREC"/>
<gate name="-74" symbol="FEMREC"/>
<gate name="-75" symbol="FEMREC"/>
<gate name="-76" symbol="FEMREC"/>
<gate name="-77" symbol="FEMREC"/>
<gate name="-78" symbol="FEMREC"/>
<gate name="-79" symbol="FEMREC"/>
<gate name="-80" symbol="FEMREC"/>
<gate name="-81" symbol="FEMREC"/>
<gate name="-82" symbol="FEMREC"/>
<gate name="-83" symbol="FEMREC"/>
<gate name="-84" symbol="FEMREC"/>
<gate name="-85" symbol="FEMREC"/>
<gate name="-86" symbol="FEMREC"/>
<gate name="-87" symbol="FEMREC"/>
<gate name="-88" symbol="FEMREC"/>
<gate name="-89" symbol="FEMREC"/>
<gate name="-90" symbol="FEMREC"/>
<gate name="-91" symbol="FEMREC"/>
<gate name="-92" symbol="FEMREC"/>
<gate name="-93" symbol="FEMREC"/>
<gate name="-94" symbol="FEMREC"/>
<gate name="-95" symbol="FEMREC"/>
<gate name="-96" symbol="FEMREC"/>
<gate name="-97" symbol="FEMREC"/>
<gate name="-98" symbol="FEMREC"/>
<gate name="-99" symbol="FEMREC"/>
<gate name="-100" symbol="FEMREC"/>
<gate name="-101" symbol="FEMREC"/>
<gate name="-102" symbol="FEMREC"/>
<gate name="-103" symbol="FEMREC"/>
<gate name="-104" symbol="FEMREC"/>
<gate name="-105" symbol="FEMREC"/>
<gate name="-106" symbol="FEMREC"/>
<gate name="-107" symbol="FEMREC"/>
<gate name="-108" symbol="FEMREC"/>
<gate name="-109" symbol="FEMREC"/>
<gate name="-110" symbol="FEMREC"/>
<gate name="-111" symbol="FEMREC"/>
<gate name="-112" symbol="FEMREC"/>
<gate name="-113" symbol="FEMREC"/>
<gate name="-114" symbol="FEMREC"/>
<gate name="-115" symbol="FEMREC"/>
<gate name="-116" symbol="FEMREC"/>
<gate name="-117" symbol="FEMREC"/>
<gate name="-118" symbol="FEMREC"/>
<gate name="-119" symbol="FEMREC"/>
<gate name="-120" symbol="FEMREC"/>
<gate name="-121" symbol="FEMREC"/>
<gate name="-122" symbol="FEMREC"/>
<gate name="-123" symbol="FEMREC"/>
<gate name="-124" symbol="FEMREC"/>
</gates>
<devices>
<device name="" package="AGP">
<connects>
<connect gate="-1" pin="P" pad="1"/>
<connect gate="-10" pin="P" pad="10"/>
<connect gate="-100" pin="P" pad="100"/>
<connect gate="-101" pin="P" pad="101"/>
<connect gate="-102" pin="P" pad="102"/>
<connect gate="-103" pin="P" pad="103"/>
<connect gate="-104" pin="P" pad="104"/>
<connect gate="-105" pin="P" pad="105"/>
<connect gate="-106" pin="P" pad="106"/>
<connect gate="-107" pin="P" pad="107"/>
<connect gate="-108" pin="P" pad="108"/>
<connect gate="-109" pin="P" pad="109"/>
<connect gate="-11" pin="P" pad="11"/>
<connect gate="-110" pin="P" pad="110"/>
<connect gate="-111" pin="P" pad="111"/>
<connect gate="-112" pin="P" pad="112"/>
<connect gate="-113" pin="P" pad="113"/>
<connect gate="-114" pin="P" pad="114"/>
<connect gate="-115" pin="P" pad="115"/>
<connect gate="-116" pin="P" pad="116"/>
<connect gate="-117" pin="P" pad="117"/>
<connect gate="-118" pin="P" pad="118"/>
<connect gate="-119" pin="P" pad="119"/>
<connect gate="-12" pin="P" pad="12"/>
<connect gate="-120" pin="P" pad="120"/>
<connect gate="-121" pin="P" pad="121"/>
<connect gate="-122" pin="P" pad="122"/>
<connect gate="-123" pin="P" pad="123"/>
<connect gate="-124" pin="P" pad="124"/>
<connect gate="-13" pin="P" pad="13"/>
<connect gate="-14" pin="P" pad="14"/>
<connect gate="-15" pin="P" pad="15"/>
<connect gate="-16" pin="P" pad="16"/>
<connect gate="-17" pin="P" pad="17"/>
<connect gate="-18" pin="P" pad="18"/>
<connect gate="-19" pin="P" pad="19"/>
<connect gate="-2" pin="P" pad="2"/>
<connect gate="-20" pin="P" pad="20"/>
<connect gate="-21" pin="P" pad="21"/>
<connect gate="-22" pin="P" pad="22"/>
<connect gate="-23" pin="P" pad="23"/>
<connect gate="-24" pin="P" pad="24"/>
<connect gate="-25" pin="P" pad="25"/>
<connect gate="-26" pin="P" pad="26"/>
<connect gate="-27" pin="P" pad="27"/>
<connect gate="-28" pin="P" pad="28"/>
<connect gate="-29" pin="P" pad="29"/>
<connect gate="-3" pin="P" pad="3"/>
<connect gate="-30" pin="P" pad="30"/>
<connect gate="-31" pin="P" pad="31"/>
<connect gate="-32" pin="P" pad="32"/>
<connect gate="-33" pin="P" pad="33"/>
<connect gate="-34" pin="P" pad="34"/>
<connect gate="-35" pin="P" pad="35"/>
<connect gate="-36" pin="P" pad="36"/>
<connect gate="-37" pin="P" pad="37"/>
<connect gate="-38" pin="P" pad="38"/>
<connect gate="-39" pin="P" pad="39"/>
<connect gate="-4" pin="P" pad="4"/>
<connect gate="-40" pin="P" pad="40"/>
<connect gate="-41" pin="P" pad="41"/>
<connect gate="-42" pin="P" pad="42"/>
<connect gate="-43" pin="P" pad="43"/>
<connect gate="-44" pin="P" pad="44"/>
<connect gate="-45" pin="P" pad="45"/>
<connect gate="-46" pin="P" pad="46"/>
<connect gate="-47" pin="P" pad="47"/>
<connect gate="-48" pin="P" pad="48"/>
<connect gate="-49" pin="P" pad="49"/>
<connect gate="-5" pin="P" pad="5"/>
<connect gate="-50" pin="P" pad="50"/>
<connect gate="-51" pin="P" pad="51"/>
<connect gate="-52" pin="P" pad="52"/>
<connect gate="-53" pin="P" pad="53"/>
<connect gate="-54" pin="P" pad="54"/>
<connect gate="-55" pin="P" pad="55"/>
<connect gate="-56" pin="P" pad="56"/>
<connect gate="-57" pin="P" pad="57"/>
<connect gate="-58" pin="P" pad="58"/>
<connect gate="-59" pin="P" pad="59"/>
<connect gate="-6" pin="P" pad="6"/>
<connect gate="-60" pin="P" pad="60"/>
<connect gate="-61" pin="P" pad="61"/>
<connect gate="-62" pin="P" pad="62"/>
<connect gate="-63" pin="P" pad="63"/>
<connect gate="-64" pin="P" pad="64"/>
<connect gate="-65" pin="P" pad="65"/>
<connect gate="-66" pin="P" pad="66"/>
<connect gate="-67" pin="P" pad="67"/>
<connect gate="-68" pin="P" pad="68"/>
<connect gate="-69" pin="P" pad="69"/>
<connect gate="-7" pin="P" pad="7"/>
<connect gate="-70" pin="P" pad="70"/>
<connect gate="-71" pin="P" pad="71"/>
<connect gate="-72" pin="P" pad="72"/>
<connect gate="-73" pin="P" pad="73"/>
<connect gate="-74" pin="P" pad="74"/>
<connect gate="-75" pin="P" pad="75"/>
<connect gate="-76" pin="P" pad="76"/>
<connect gate="-77" pin="P" pad="77"/>
<connect gate="-78" pin="P" pad="78"/>
<connect gate="-79" pin="P" pad="79"/>
<connect gate="-8" pin="P" pad="8"/>
<connect gate="-80" pin="P" pad="80"/>
<connect gate="-81" pin="P" pad="81"/>
<connect gate="-82" pin="P" pad="82"/>
<connect gate="-83" pin="P" pad="83"/>
<connect gate="-84" pin="P" pad="84"/>
<connect gate="-85" pin="P" pad="85"/>
<connect gate="-86" pin="P" pad="86"/>
<connect gate="-87" pin="P" pad="87"/>
<connect gate="-88" pin="P" pad="88"/>
<connect gate="-89" pin="P" pad="89"/>
<connect gate="-9" pin="P" pad="9"/>
<connect gate="-90" pin="P" pad="90"/>
<connect gate="-91" pin="P" pad="91"/>
<connect gate="-92" pin="P" pad="92"/>
<connect gate="-93" pin="P" pad="93"/>
<connect gate="-94" pin="P" pad="94"/>
<connect gate="-95" pin="P" pad="95"/>
<connect gate="-96" pin="P" pad="96"/>
<connect gate="-97" pin="P" pad="97"/>
<connect gate="-98" pin="P" pad="98"/>
<connect gate="-99" pin="P" pad="99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SLOT" package="AGP-SLOT">
<connects>
<connect gate="-1" pin="P" pad="1"/>
<connect gate="-10" pin="P" pad="10"/>
<connect gate="-100" pin="P" pad="100"/>
<connect gate="-101" pin="P" pad="101"/>
<connect gate="-102" pin="P" pad="102"/>
<connect gate="-103" pin="P" pad="103"/>
<connect gate="-104" pin="P" pad="104"/>
<connect gate="-105" pin="P" pad="105"/>
<connect gate="-106" pin="P" pad="106"/>
<connect gate="-107" pin="P" pad="107"/>
<connect gate="-108" pin="P" pad="108"/>
<connect gate="-109" pin="P" pad="109"/>
<connect gate="-11" pin="P" pad="11"/>
<connect gate="-110" pin="P" pad="110"/>
<connect gate="-111" pin="P" pad="111"/>
<connect gate="-112" pin="P" pad="112"/>
<connect gate="-113" pin="P" pad="113"/>
<connect gate="-114" pin="P" pad="114"/>
<connect gate="-115" pin="P" pad="115"/>
<connect gate="-116" pin="P" pad="116"/>
<connect gate="-117" pin="P" pad="117"/>
<connect gate="-118" pin="P" pad="118"/>
<connect gate="-119" pin="P" pad="119"/>
<connect gate="-12" pin="P" pad="12"/>
<connect gate="-120" pin="P" pad="120"/>
<connect gate="-121" pin="P" pad="121"/>
<connect gate="-122" pin="P" pad="122"/>
<connect gate="-123" pin="P" pad="123"/>
<connect gate="-124" pin="P" pad="124"/>
<connect gate="-13" pin="P" pad="13"/>
<connect gate="-14" pin="P" pad="14"/>
<connect gate="-15" pin="P" pad="15"/>
<connect gate="-16" pin="P" pad="16"/>
<connect gate="-17" pin="P" pad="17"/>
<connect gate="-18" pin="P" pad="18"/>
<connect gate="-19" pin="P" pad="19"/>
<connect gate="-2" pin="P" pad="2"/>
<connect gate="-20" pin="P" pad="20"/>
<connect gate="-21" pin="P" pad="21"/>
<connect gate="-22" pin="P" pad="22"/>
<connect gate="-23" pin="P" pad="23"/>
<connect gate="-24" pin="P" pad="24"/>
<connect gate="-25" pin="P" pad="25"/>
<connect gate="-26" pin="P" pad="26"/>
<connect gate="-27" pin="P" pad="27"/>
<connect gate="-28" pin="P" pad="28"/>
<connect gate="-29" pin="P" pad="29"/>
<connect gate="-3" pin="P" pad="3"/>
<connect gate="-30" pin="P" pad="30"/>
<connect gate="-31" pin="P" pad="31"/>
<connect gate="-32" pin="P" pad="32"/>
<connect gate="-33" pin="P" pad="33"/>
<connect gate="-34" pin="P" pad="34"/>
<connect gate="-35" pin="P" pad="35"/>
<connect gate="-36" pin="P" pad="36"/>
<connect gate="-37" pin="P" pad="37"/>
<connect gate="-38" pin="P" pad="38"/>
<connect gate="-39" pin="P" pad="39"/>
<connect gate="-4" pin="P" pad="4"/>
<connect gate="-40" pin="P" pad="40"/>
<connect gate="-41" pin="P" pad="41"/>
<connect gate="-42" pin="P" pad="42"/>
<connect gate="-43" pin="P" pad="43"/>
<connect gate="-44" pin="P" pad="44"/>
<connect gate="-45" pin="P" pad="45"/>
<connect gate="-46" pin="P" pad="46"/>
<connect gate="-47" pin="P" pad="47"/>
<connect gate="-48" pin="P" pad="48"/>
<connect gate="-49" pin="P" pad="49"/>
<connect gate="-5" pin="P" pad="5"/>
<connect gate="-50" pin="P" pad="50"/>
<connect gate="-51" pin="P" pad="51"/>
<connect gate="-52" pin="P" pad="52"/>
<connect gate="-53" pin="P" pad="53"/>
<connect gate="-54" pin="P" pad="54"/>
<connect gate="-55" pin="P" pad="55"/>
<connect gate="-56" pin="P" pad="56"/>
<connect gate="-57" pin="P" pad="57"/>
<connect gate="-58" pin="P" pad="58"/>
<connect gate="-59" pin="P" pad="59"/>
<connect gate="-6" pin="P" pad="6"/>
<connect gate="-60" pin="P" pad="60"/>
<connect gate="-61" pin="P" pad="61"/>
<connect gate="-62" pin="P" pad="62"/>
<connect gate="-63" pin="P" pad="63"/>
<connect gate="-64" pin="P" pad="64"/>
<connect gate="-65" pin="P" pad="65"/>
<connect gate="-66" pin="P" pad="66"/>
<connect gate="-67" pin="P" pad="67"/>
<connect gate="-68" pin="P" pad="68"/>
<connect gate="-69" pin="P" pad="69"/>
<connect gate="-7" pin="P" pad="7"/>
<connect gate="-70" pin="P" pad="70"/>
<connect gate="-71" pin="P" pad="71"/>
<connect gate="-72" pin="P" pad="72"/>
<connect gate="-73" pin="P" pad="73"/>
<connect gate="-74" pin="P" pad="74"/>
<connect gate="-75" pin="P" pad="75"/>
<connect gate="-76" pin="P" pad="76"/>
<connect gate="-77" pin="P" pad="77"/>
<connect gate="-78" pin="P" pad="78"/>
<connect gate="-79" pin="P" pad="79"/>
<connect gate="-8" pin="P" pad="8"/>
<connect gate="-80" pin="P" pad="80"/>
<connect gate="-81" pin="P" pad="81"/>
<connect gate="-82" pin="P" pad="82"/>
<connect gate="-83" pin="P" pad="83"/>
<connect gate="-84" pin="P" pad="84"/>
<connect gate="-85" pin="P" pad="85"/>
<connect gate="-86" pin="P" pad="86"/>
<connect gate="-87" pin="P" pad="87"/>
<connect gate="-88" pin="P" pad="88"/>
<connect gate="-89" pin="P" pad="89"/>
<connect gate="-9" pin="P" pad="9"/>
<connect gate="-90" pin="P" pad="90"/>
<connect gate="-91" pin="P" pad="91"/>
<connect gate="-92" pin="P" pad="92"/>
<connect gate="-93" pin="P" pad="93"/>
<connect gate="-94" pin="P" pad="94"/>
<connect gate="-95" pin="P" pad="95"/>
<connect gate="-96" pin="P" pad="96"/>
<connect gate="-97" pin="P" pad="97"/>
<connect gate="-98" pin="P" pad="98"/>
<connect gate="-99" pin="P" pad="99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AGP-SLOT" prefix="X">
<description>&lt;b&gt;AGP Slot&lt;/b&gt; AMP connctor 145263 &amp;gt;PCT-GF40&amp;lt;&lt;p&gt;
124 Position 1mm, card edge connector&lt;br&gt;
Drawing No: C-145263&lt;br&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_145263_H.pdf</description>
<gates>
<gate name="-1" symbol="MALEVAL"/>
<gate name="-2" symbol="MALEVAL"/>
<gate name="-3" symbol="MALE"/>
<gate name="-4" symbol="MALE"/>
<gate name="-5" symbol="MALE"/>
<gate name="-6" symbol="MALE"/>
<gate name="-7" symbol="MALE"/>
<gate name="-8" symbol="MALE"/>
<gate name="-9" symbol="MALE"/>
<gate name="-10" symbol="MALE"/>
<gate name="-11" symbol="MALE"/>
<gate name="-12" symbol="MALE"/>
<gate name="-13" symbol="MALE"/>
<gate name="-14" symbol="MALE"/>
<gate name="-15" symbol="MALE"/>
<gate name="-16" symbol="MALE"/>
<gate name="-17" symbol="MALE"/>
<gate name="-18" symbol="MALE"/>
<gate name="-19" symbol="MALE"/>
<gate name="-20" symbol="MALE"/>
<gate name="-21" symbol="MALE"/>
<gate name="-22" symbol="MALE"/>
<gate name="-23" symbol="MALE"/>
<gate name="-24" symbol="MALE"/>
<gate name="-25" symbol="MALE"/>
<gate name="-26" symbol="MALE"/>
<gate name="-27" symbol="MALE"/>
<gate name="-28" symbol="MALE"/>
<gate name="-29" symbol="MALE"/>
<gate name="-30" symbol="MALE"/>
<gate name="-31" symbol="MALE"/>
<gate name="-32" symbol="MALE"/>
<gate name="-33" symbol="MALE"/>
<gate name="-34" symbol="MALE"/>
<gate name="-35" symbol="MALE"/>
<gate name="-36" symbol="MALE"/>
<gate name="-37" symbol="MALE"/>
<gate name="-38" symbol="MALE"/>
<gate name="-39" symbol="MALE"/>
<gate name="-40" symbol="MALE"/>
<gate name="-41" symbol="MALE"/>
<gate name="-42" symbol="MALE"/>
<gate name="-43" symbol="MALE"/>
<gate name="-44" symbol="MALE"/>
<gate name="-45" symbol="MALE"/>
<gate name="-46" symbol="MALE"/>
<gate name="-47" symbol="MALE"/>
<gate name="-48" symbol="MALE"/>
<gate name="-49" symbol="MALE"/>
<gate name="-50" symbol="MALE"/>
<gate name="-51" symbol="MALE"/>
<gate name="-52" symbol="MALE"/>
<gate name="-53" symbol="MALE"/>
<gate name="-54" symbol="MALE"/>
<gate name="-55" symbol="MALE"/>
<gate name="-56" symbol="MALE"/>
<gate name="-57" symbol="MALE"/>
<gate name="-58" symbol="MALE"/>
<gate name="-59" symbol="MALE"/>
<gate name="-60" symbol="MALE"/>
<gate name="-61" symbol="MALE"/>
<gate name="-62" symbol="MALE"/>
<gate name="-63" symbol="MALE"/>
<gate name="-64" symbol="MALE"/>
<gate name="-65" symbol="MALE"/>
<gate name="-66" symbol="MALE"/>
<gate name="-67" symbol="MALE"/>
<gate name="-68" symbol="MALE"/>
<gate name="-69" symbol="MALE"/>
<gate name="-70" symbol="MALE"/>
<gate name="-71" symbol="MALE"/>
<gate name="-72" symbol="MALE"/>
<gate name="-73" symbol="MALE"/>
<gate name="-74" symbol="MALE"/>
<gate name="-75" symbol="MALE"/>
<gate name="-76" symbol="MALE"/>
<gate name="-77" symbol="MALE"/>
<gate name="-78" symbol="MALE"/>
<gate name="-79" symbol="MALE"/>
<gate name="-80" symbol="MALE"/>
<gate name="-81" symbol="MALE"/>
<gate name="-82" symbol="MALE"/>
<gate name="-83" symbol="MALE"/>
<gate name="-84" symbol="MALE"/>
<gate name="-85" symbol="MALE"/>
<gate name="-86" symbol="MALE"/>
<gate name="-87" symbol="MALE"/>
<gate name="-88" symbol="MALE"/>
<gate name="-89" symbol="MALE"/>
<gate name="-90" symbol="MALE"/>
<gate name="-91" symbol="MALE"/>
<gate name="-92" symbol="MALE"/>
<gate name="-93" symbol="MALE"/>
<gate name="-94" symbol="MALE"/>
<gate name="-95" symbol="MALE"/>
<gate name="-96" symbol="MALE"/>
<gate name="-97" symbol="MALE"/>
<gate name="-98" symbol="MALE"/>
<gate name="-99" symbol="MALE"/>
<gate name="-100" symbol="MALE"/>
<gate name="-101" symbol="MALE"/>
<gate name="-102" symbol="MALE"/>
<gate name="-103" symbol="MALE"/>
<gate name="-104" symbol="MALE"/>
<gate name="-105" symbol="MALE"/>
<gate name="-106" symbol="MALE"/>
<gate name="-107" symbol="MALE"/>
<gate name="-108" symbol="MALE"/>
<gate name="-109" symbol="MALE"/>
<gate name="-110" symbol="MALE"/>
<gate name="-111" symbol="MALE"/>
<gate name="-112" symbol="MALE"/>
<gate name="-113" symbol="MALE"/>
<gate name="-114" symbol="MALE"/>
<gate name="-115" symbol="MALE"/>
<gate name="-116" symbol="MALE"/>
<gate name="-117" symbol="MALE"/>
<gate name="-118" symbol="MALE"/>
<gate name="-119" symbol="MALE"/>
<gate name="-120" symbol="MALE"/>
<gate name="-121" symbol="MALE"/>
<gate name="-122" symbol="MALE"/>
<gate name="-123" symbol="MALE"/>
<gate name="-124" symbol="MALE"/>
</gates>
<devices>
<device name="" package="AGP-SLOT">
<connects>
<connect gate="-1" pin="P" pad="1"/>
<connect gate="-10" pin="P" pad="10"/>
<connect gate="-100" pin="P" pad="100"/>
<connect gate="-101" pin="P" pad="101"/>
<connect gate="-102" pin="P" pad="102"/>
<connect gate="-103" pin="P" pad="103"/>
<connect gate="-104" pin="P" pad="104"/>
<connect gate="-105" pin="P" pad="105"/>
<connect gate="-106" pin="P" pad="106"/>
<connect gate="-107" pin="P" pad="107"/>
<connect gate="-108" pin="P" pad="108"/>
<connect gate="-109" pin="P" pad="109"/>
<connect gate="-11" pin="P" pad="11"/>
<connect gate="-110" pin="P" pad="110"/>
<connect gate="-111" pin="P" pad="111"/>
<connect gate="-112" pin="P" pad="112"/>
<connect gate="-113" pin="P" pad="113"/>
<connect gate="-114" pin="P" pad="114"/>
<connect gate="-115" pin="P" pad="115"/>
<connect gate="-116" pin="P" pad="116"/>
<connect gate="-117" pin="P" pad="117"/>
<connect gate="-118" pin="P" pad="118"/>
<connect gate="-119" pin="P" pad="119"/>
<connect gate="-12" pin="P" pad="12"/>
<connect gate="-120" pin="P" pad="120"/>
<connect gate="-121" pin="P" pad="121"/>
<connect gate="-122" pin="P" pad="122"/>
<connect gate="-123" pin="P" pad="123"/>
<connect gate="-124" pin="P" pad="124"/>
<connect gate="-13" pin="P" pad="13"/>
<connect gate="-14" pin="P" pad="14"/>
<connect gate="-15" pin="P" pad="15"/>
<connect gate="-16" pin="P" pad="16"/>
<connect gate="-17" pin="P" pad="17"/>
<connect gate="-18" pin="P" pad="18"/>
<connect gate="-19" pin="P" pad="19"/>
<connect gate="-2" pin="P" pad="2"/>
<connect gate="-20" pin="P" pad="20"/>
<connect gate="-21" pin="P" pad="21"/>
<connect gate="-22" pin="P" pad="22"/>
<connect gate="-23" pin="P" pad="23"/>
<connect gate="-24" pin="P" pad="24"/>
<connect gate="-25" pin="P" pad="25"/>
<connect gate="-26" pin="P" pad="26"/>
<connect gate="-27" pin="P" pad="27"/>
<connect gate="-28" pin="P" pad="28"/>
<connect gate="-29" pin="P" pad="29"/>
<connect gate="-3" pin="P" pad="3"/>
<connect gate="-30" pin="P" pad="30"/>
<connect gate="-31" pin="P" pad="31"/>
<connect gate="-32" pin="P" pad="32"/>
<connect gate="-33" pin="P" pad="33"/>
<connect gate="-34" pin="P" pad="34"/>
<connect gate="-35" pin="P" pad="35"/>
<connect gate="-36" pin="P" pad="36"/>
<connect gate="-37" pin="P" pad="37"/>
<connect gate="-38" pin="P" pad="38"/>
<connect gate="-39" pin="P" pad="39"/>
<connect gate="-4" pin="P" pad="4"/>
<connect gate="-40" pin="P" pad="40"/>
<connect gate="-41" pin="P" pad="41"/>
<connect gate="-42" pin="P" pad="42"/>
<connect gate="-43" pin="P" pad="43"/>
<connect gate="-44" pin="P" pad="44"/>
<connect gate="-45" pin="P" pad="45"/>
<connect gate="-46" pin="P" pad="46"/>
<connect gate="-47" pin="P" pad="47"/>
<connect gate="-48" pin="P" pad="48"/>
<connect gate="-49" pin="P" pad="49"/>
<connect gate="-5" pin="P" pad="5"/>
<connect gate="-50" pin="P" pad="50"/>
<connect gate="-51" pin="P" pad="51"/>
<connect gate="-52" pin="P" pad="52"/>
<connect gate="-53" pin="P" pad="53"/>
<connect gate="-54" pin="P" pad="54"/>
<connect gate="-55" pin="P" pad="55"/>
<connect gate="-56" pin="P" pad="56"/>
<connect gate="-57" pin="P" pad="57"/>
<connect gate="-58" pin="P" pad="58"/>
<connect gate="-59" pin="P" pad="59"/>
<connect gate="-6" pin="P" pad="6"/>
<connect gate="-60" pin="P" pad="60"/>
<connect gate="-61" pin="P" pad="61"/>
<connect gate="-62" pin="P" pad="62"/>
<connect gate="-63" pin="P" pad="63"/>
<connect gate="-64" pin="P" pad="64"/>
<connect gate="-65" pin="P" pad="65"/>
<connect gate="-66" pin="P" pad="66"/>
<connect gate="-67" pin="P" pad="67"/>
<connect gate="-68" pin="P" pad="68"/>
<connect gate="-69" pin="P" pad="69"/>
<connect gate="-7" pin="P" pad="7"/>
<connect gate="-70" pin="P" pad="70"/>
<connect gate="-71" pin="P" pad="71"/>
<connect gate="-72" pin="P" pad="72"/>
<connect gate="-73" pin="P" pad="73"/>
<connect gate="-74" pin="P" pad="74"/>
<connect gate="-75" pin="P" pad="75"/>
<connect gate="-76" pin="P" pad="76"/>
<connect gate="-77" pin="P" pad="77"/>
<connect gate="-78" pin="P" pad="78"/>
<connect gate="-79" pin="P" pad="79"/>
<connect gate="-8" pin="P" pad="8"/>
<connect gate="-80" pin="P" pad="80"/>
<connect gate="-81" pin="P" pad="81"/>
<connect gate="-82" pin="P" pad="82"/>
<connect gate="-83" pin="P" pad="83"/>
<connect gate="-84" pin="P" pad="84"/>
<connect gate="-85" pin="P" pad="85"/>
<connect gate="-86" pin="P" pad="86"/>
<connect gate="-87" pin="P" pad="87"/>
<connect gate="-88" pin="P" pad="88"/>
<connect gate="-89" pin="P" pad="89"/>
<connect gate="-9" pin="P" pad="9"/>
<connect gate="-90" pin="P" pad="90"/>
<connect gate="-91" pin="P" pad="91"/>
<connect gate="-92" pin="P" pad="92"/>
<connect gate="-93" pin="P" pad="93"/>
<connect gate="-94" pin="P" pad="94"/>
<connect gate="-95" pin="P" pad="95"/>
<connect gate="-96" pin="P" pad="96"/>
<connect gate="-97" pin="P" pad="97"/>
<connect gate="-98" pin="P" pad="98"/>
<connect gate="-99" pin="P" pad="99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AGP_UC" prefix="X">
<description>&lt;b&gt;AGP:UC Slot&lt;/b&gt; AMP connctor 145376 &amp;gt;PCT-GF40&amp;lt; &lt;p&gt;
132 Position 1mm, card edge connector&lt;br&gt;
Drawing No: C-145263&lt;br&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_145376_D.pdf</description>
<gates>
<gate name="-1" symbol="FEMRVAL"/>
<gate name="-2" symbol="FEMRVAL"/>
<gate name="-3" symbol="FEMREC"/>
<gate name="-4" symbol="FEMREC"/>
<gate name="-5" symbol="FEMREC"/>
<gate name="-6" symbol="FEMREC"/>
<gate name="-7" symbol="FEMREC"/>
<gate name="-8" symbol="FEMREC"/>
<gate name="-9" symbol="FEMREC"/>
<gate name="-10" symbol="FEMREC"/>
<gate name="-11" symbol="FEMREC"/>
<gate name="-12" symbol="FEMREC"/>
<gate name="-13" symbol="FEMREC"/>
<gate name="-14" symbol="FEMREC"/>
<gate name="-15" symbol="FEMREC"/>
<gate name="-16" symbol="FEMREC"/>
<gate name="-17" symbol="FEMREC"/>
<gate name="-18" symbol="FEMREC"/>
<gate name="-19" symbol="FEMREC"/>
<gate name="-20" symbol="FEMREC"/>
<gate name="-21" symbol="FEMREC"/>
<gate name="-22" symbol="FEMREC"/>
<gate name="-23" symbol="FEMREC"/>
<gate name="-24" symbol="FEMREC"/>
<gate name="-25" symbol="FEMREC"/>
<gate name="-26" symbol="FEMREC"/>
<gate name="-27" symbol="FEMREC"/>
<gate name="-28" symbol="FEMREC"/>
<gate name="-29" symbol="FEMREC"/>
<gate name="-30" symbol="FEMREC"/>
<gate name="-31" symbol="FEMREC"/>
<gate name="-32" symbol="FEMREC"/>
<gate name="-33" symbol="FEMREC"/>
<gate name="-34" symbol="FEMREC"/>
<gate name="-35" symbol="FEMREC"/>
<gate name="-36" symbol="FEMREC"/>
<gate name="-37" symbol="FEMREC"/>
<gate name="-38" symbol="FEMREC"/>
<gate name="-39" symbol="FEMREC"/>
<gate name="-40" symbol="FEMREC"/>
<gate name="-41" symbol="FEMREC"/>
<gate name="-42" symbol="FEMREC"/>
<gate name="-43" symbol="FEMREC"/>
<gate name="-44" symbol="FEMREC"/>
<gate name="-45" symbol="FEMREC"/>
<gate name="-46" symbol="FEMREC"/>
<gate name="-47" symbol="FEMREC"/>
<gate name="-48" symbol="FEMREC"/>
<gate name="-49" symbol="FEMREC"/>
<gate name="-50" symbol="FEMREC"/>
<gate name="-51" symbol="FEMREC"/>
<gate name="-52" symbol="FEMREC"/>
<gate name="-53" symbol="FEMREC"/>
<gate name="-54" symbol="FEMREC"/>
<gate name="-55" symbol="FEMREC"/>
<gate name="-56" symbol="FEMREC"/>
<gate name="-57" symbol="FEMREC"/>
<gate name="-58" symbol="FEMREC"/>
<gate name="-59" symbol="FEMREC"/>
<gate name="-60" symbol="FEMREC"/>
<gate name="-61" symbol="FEMREC"/>
<gate name="-62" symbol="FEMREC"/>
<gate name="-63" symbol="FEMREC"/>
<gate name="-64" symbol="FEMREC"/>
<gate name="-65" symbol="FEMREC"/>
<gate name="-66" symbol="FEMREC"/>
<gate name="-67" symbol="FEMREC"/>
<gate name="-68" symbol="FEMREC"/>
<gate name="-69" symbol="FEMREC"/>
<gate name="-70" symbol="FEMREC"/>
<gate name="-71" symbol="FEMREC"/>
<gate name="-72" symbol="FEMREC"/>
<gate name="-73" symbol="FEMREC"/>
<gate name="-74" symbol="FEMREC"/>
<gate name="-75" symbol="FEMREC"/>
<gate name="-76" symbol="FEMREC"/>
<gate name="-77" symbol="FEMREC"/>
<gate name="-78" symbol="FEMREC"/>
<gate name="-79" symbol="FEMREC"/>
<gate name="-80" symbol="FEMREC"/>
<gate name="-81" symbol="FEMREC"/>
<gate name="-82" symbol="FEMREC"/>
<gate name="-83" symbol="FEMREC"/>
<gate name="-84" symbol="FEMREC"/>
<gate name="-85" symbol="FEMREC"/>
<gate name="-86" symbol="FEMREC"/>
<gate name="-87" symbol="FEMREC"/>
<gate name="-88" symbol="FEMREC"/>
<gate name="-89" symbol="FEMREC"/>
<gate name="-90" symbol="FEMREC"/>
<gate name="-91" symbol="FEMREC"/>
<gate name="-92" symbol="FEMREC"/>
<gate name="-93" symbol="FEMREC"/>
<gate name="-94" symbol="FEMREC"/>
<gate name="-95" symbol="FEMREC"/>
<gate name="-96" symbol="FEMREC"/>
<gate name="-97" symbol="FEMREC"/>
<gate name="-98" symbol="FEMREC"/>
<gate name="-99" symbol="FEMREC"/>
<gate name="-100" symbol="FEMREC"/>
<gate name="-101" symbol="FEMREC"/>
<gate name="-102" symbol="FEMREC"/>
<gate name="-103" symbol="FEMREC"/>
<gate name="-104" symbol="FEMREC"/>
<gate name="-105" symbol="FEMREC"/>
<gate name="-106" symbol="FEMREC"/>
<gate name="-107" symbol="FEMREC"/>
<gate name="-108" symbol="FEMREC"/>
<gate name="-109" symbol="FEMREC"/>
<gate name="-110" symbol="FEMREC"/>
<gate name="-111" symbol="FEMREC"/>
<gate name="-112" symbol="FEMREC"/>
<gate name="-113" symbol="FEMREC"/>
<gate name="-114" symbol="FEMREC"/>
<gate name="-115" symbol="FEMREC"/>
<gate name="-116" symbol="FEMREC"/>
<gate name="-117" symbol="FEMREC"/>
<gate name="-118" symbol="FEMREC"/>
<gate name="-119" symbol="FEMREC"/>
<gate name="-120" symbol="FEMREC"/>
<gate name="-121" symbol="FEMREC"/>
<gate name="-122" symbol="FEMREC"/>
<gate name="-123" symbol="FEMREC"/>
<gate name="-124" symbol="FEMREC"/>
<gate name="-125" symbol="FEMREC"/>
<gate name="-126" symbol="FEMREC"/>
<gate name="-127" symbol="FEMREC"/>
<gate name="-128" symbol="FEMREC"/>
<gate name="-129" symbol="FEMREC"/>
<gate name="-130" symbol="FEMREC"/>
<gate name="-131" symbol="FEMREC"/>
<gate name="-132" symbol="FEMREC"/>
</gates>
<devices>
<device name="" package="AGP_UC">
<connects>
<connect gate="-1" pin="P" pad="1"/>
<connect gate="-10" pin="P" pad="10"/>
<connect gate="-100" pin="P" pad="100"/>
<connect gate="-101" pin="P" pad="101"/>
<connect gate="-102" pin="P" pad="102"/>
<connect gate="-103" pin="P" pad="103"/>
<connect gate="-104" pin="P" pad="104"/>
<connect gate="-105" pin="P" pad="105"/>
<connect gate="-106" pin="P" pad="106"/>
<connect gate="-107" pin="P" pad="107"/>
<connect gate="-108" pin="P" pad="108"/>
<connect gate="-109" pin="P" pad="109"/>
<connect gate="-11" pin="P" pad="11"/>
<connect gate="-110" pin="P" pad="110"/>
<connect gate="-111" pin="P" pad="111"/>
<connect gate="-112" pin="P" pad="112"/>
<connect gate="-113" pin="P" pad="113"/>
<connect gate="-114" pin="P" pad="114"/>
<connect gate="-115" pin="P" pad="115"/>
<connect gate="-116" pin="P" pad="116"/>
<connect gate="-117" pin="P" pad="117"/>
<connect gate="-118" pin="P" pad="118"/>
<connect gate="-119" pin="P" pad="119"/>
<connect gate="-12" pin="P" pad="12"/>
<connect gate="-120" pin="P" pad="120"/>
<connect gate="-121" pin="P" pad="121"/>
<connect gate="-122" pin="P" pad="122"/>
<connect gate="-123" pin="P" pad="123"/>
<connect gate="-124" pin="P" pad="124"/>
<connect gate="-125" pin="P" pad="125"/>
<connect gate="-126" pin="P" pad="126"/>
<connect gate="-127" pin="P" pad="127"/>
<connect gate="-128" pin="P" pad="128"/>
<connect gate="-129" pin="P" pad="129"/>
<connect gate="-13" pin="P" pad="13"/>
<connect gate="-130" pin="P" pad="130"/>
<connect gate="-131" pin="P" pad="131"/>
<connect gate="-132" pin="P" pad="132"/>
<connect gate="-14" pin="P" pad="14"/>
<connect gate="-15" pin="P" pad="15"/>
<connect gate="-16" pin="P" pad="16"/>
<connect gate="-17" pin="P" pad="17"/>
<connect gate="-18" pin="P" pad="18"/>
<connect gate="-19" pin="P" pad="19"/>
<connect gate="-2" pin="P" pad="2"/>
<connect gate="-20" pin="P" pad="20"/>
<connect gate="-21" pin="P" pad="21"/>
<connect gate="-22" pin="P" pad="22"/>
<connect gate="-23" pin="P" pad="23"/>
<connect gate="-24" pin="P" pad="24"/>
<connect gate="-25" pin="P" pad="25"/>
<connect gate="-26" pin="P" pad="26"/>
<connect gate="-27" pin="P" pad="27"/>
<connect gate="-28" pin="P" pad="28"/>
<connect gate="-29" pin="P" pad="29"/>
<connect gate="-3" pin="P" pad="3"/>
<connect gate="-30" pin="P" pad="30"/>
<connect gate="-31" pin="P" pad="31"/>
<connect gate="-32" pin="P" pad="32"/>
<connect gate="-33" pin="P" pad="33"/>
<connect gate="-34" pin="P" pad="34"/>
<connect gate="-35" pin="P" pad="35"/>
<connect gate="-36" pin="P" pad="36"/>
<connect gate="-37" pin="P" pad="37"/>
<connect gate="-38" pin="P" pad="38"/>
<connect gate="-39" pin="P" pad="39"/>
<connect gate="-4" pin="P" pad="4"/>
<connect gate="-40" pin="P" pad="40"/>
<connect gate="-41" pin="P" pad="41"/>
<connect gate="-42" pin="P" pad="42"/>
<connect gate="-43" pin="P" pad="43"/>
<connect gate="-44" pin="P" pad="44"/>
<connect gate="-45" pin="P" pad="45"/>
<connect gate="-46" pin="P" pad="46"/>
<connect gate="-47" pin="P" pad="47"/>
<connect gate="-48" pin="P" pad="48"/>
<connect gate="-49" pin="P" pad="49"/>
<connect gate="-5" pin="P" pad="5"/>
<connect gate="-50" pin="P" pad="50"/>
<connect gate="-51" pin="P" pad="51"/>
<connect gate="-52" pin="P" pad="52"/>
<connect gate="-53" pin="P" pad="53"/>
<connect gate="-54" pin="P" pad="54"/>
<connect gate="-55" pin="P" pad="55"/>
<connect gate="-56" pin="P" pad="56"/>
<connect gate="-57" pin="P" pad="57"/>
<connect gate="-58" pin="P" pad="58"/>
<connect gate="-59" pin="P" pad="59"/>
<connect gate="-6" pin="P" pad="6"/>
<connect gate="-60" pin="P" pad="60"/>
<connect gate="-61" pin="P" pad="61"/>
<connect gate="-62" pin="P" pad="62"/>
<connect gate="-63" pin="P" pad="63"/>
<connect gate="-64" pin="P" pad="64"/>
<connect gate="-65" pin="P" pad="65"/>
<connect gate="-66" pin="P" pad="66"/>
<connect gate="-67" pin="P" pad="67"/>
<connect gate="-68" pin="P" pad="68"/>
<connect gate="-69" pin="P" pad="69"/>
<connect gate="-7" pin="P" pad="7"/>
<connect gate="-70" pin="P" pad="70"/>
<connect gate="-71" pin="P" pad="71"/>
<connect gate="-72" pin="P" pad="72"/>
<connect gate="-73" pin="P" pad="73"/>
<connect gate="-74" pin="P" pad="74"/>
<connect gate="-75" pin="P" pad="75"/>
<connect gate="-76" pin="P" pad="76"/>
<connect gate="-77" pin="P" pad="77"/>
<connect gate="-78" pin="P" pad="78"/>
<connect gate="-79" pin="P" pad="79"/>
<connect gate="-8" pin="P" pad="8"/>
<connect gate="-80" pin="P" pad="80"/>
<connect gate="-81" pin="P" pad="81"/>
<connect gate="-82" pin="P" pad="82"/>
<connect gate="-83" pin="P" pad="83"/>
<connect gate="-84" pin="P" pad="84"/>
<connect gate="-85" pin="P" pad="85"/>
<connect gate="-86" pin="P" pad="86"/>
<connect gate="-87" pin="P" pad="87"/>
<connect gate="-88" pin="P" pad="88"/>
<connect gate="-89" pin="P" pad="89"/>
<connect gate="-9" pin="P" pad="9"/>
<connect gate="-90" pin="P" pad="90"/>
<connect gate="-91" pin="P" pad="91"/>
<connect gate="-92" pin="P" pad="92"/>
<connect gate="-93" pin="P" pad="93"/>
<connect gate="-94" pin="P" pad="94"/>
<connect gate="-95" pin="P" pad="95"/>
<connect gate="-96" pin="P" pad="96"/>
<connect gate="-97" pin="P" pad="97"/>
<connect gate="-98" pin="P" pad="98"/>
<connect gate="-99" pin="P" pad="99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SLOT" package="AGP_UC-SLOT">
<connects>
<connect gate="-1" pin="P" pad="1"/>
<connect gate="-10" pin="P" pad="10"/>
<connect gate="-100" pin="P" pad="100"/>
<connect gate="-101" pin="P" pad="101"/>
<connect gate="-102" pin="P" pad="102"/>
<connect gate="-103" pin="P" pad="103"/>
<connect gate="-104" pin="P" pad="104"/>
<connect gate="-105" pin="P" pad="105"/>
<connect gate="-106" pin="P" pad="106"/>
<connect gate="-107" pin="P" pad="107"/>
<connect gate="-108" pin="P" pad="108"/>
<connect gate="-109" pin="P" pad="109"/>
<connect gate="-11" pin="P" pad="11"/>
<connect gate="-110" pin="P" pad="110"/>
<connect gate="-111" pin="P" pad="111"/>
<connect gate="-112" pin="P" pad="112"/>
<connect gate="-113" pin="P" pad="113"/>
<connect gate="-114" pin="P" pad="114"/>
<connect gate="-115" pin="P" pad="115"/>
<connect gate="-116" pin="P" pad="116"/>
<connect gate="-117" pin="P" pad="117"/>
<connect gate="-118" pin="P" pad="118"/>
<connect gate="-119" pin="P" pad="119"/>
<connect gate="-12" pin="P" pad="12"/>
<connect gate="-120" pin="P" pad="120"/>
<connect gate="-121" pin="P" pad="121"/>
<connect gate="-122" pin="P" pad="122"/>
<connect gate="-123" pin="P" pad="123"/>
<connect gate="-124" pin="P" pad="124"/>
<connect gate="-125" pin="P" pad="125"/>
<connect gate="-126" pin="P" pad="126"/>
<connect gate="-127" pin="P" pad="127"/>
<connect gate="-128" pin="P" pad="128"/>
<connect gate="-129" pin="P" pad="129"/>
<connect gate="-13" pin="P" pad="13"/>
<connect gate="-130" pin="P" pad="130"/>
<connect gate="-131" pin="P" pad="131"/>
<connect gate="-132" pin="P" pad="132"/>
<connect gate="-14" pin="P" pad="14"/>
<connect gate="-15" pin="P" pad="15"/>
<connect gate="-16" pin="P" pad="16"/>
<connect gate="-17" pin="P" pad="17"/>
<connect gate="-18" pin="P" pad="18"/>
<connect gate="-19" pin="P" pad="19"/>
<connect gate="-2" pin="P" pad="2"/>
<connect gate="-20" pin="P" pad="20"/>
<connect gate="-21" pin="P" pad="21"/>
<connect gate="-22" pin="P" pad="22"/>
<connect gate="-23" pin="P" pad="23"/>
<connect gate="-24" pin="P" pad="24"/>
<connect gate="-25" pin="P" pad="25"/>
<connect gate="-26" pin="P" pad="26"/>
<connect gate="-27" pin="P" pad="27"/>
<connect gate="-28" pin="P" pad="28"/>
<connect gate="-29" pin="P" pad="29"/>
<connect gate="-3" pin="P" pad="3"/>
<connect gate="-30" pin="P" pad="30"/>
<connect gate="-31" pin="P" pad="31"/>
<connect gate="-32" pin="P" pad="32"/>
<connect gate="-33" pin="P" pad="33"/>
<connect gate="-34" pin="P" pad="34"/>
<connect gate="-35" pin="P" pad="35"/>
<connect gate="-36" pin="P" pad="36"/>
<connect gate="-37" pin="P" pad="37"/>
<connect gate="-38" pin="P" pad="38"/>
<connect gate="-39" pin="P" pad="39"/>
<connect gate="-4" pin="P" pad="4"/>
<connect gate="-40" pin="P" pad="40"/>
<connect gate="-41" pin="P" pad="41"/>
<connect gate="-42" pin="P" pad="42"/>
<connect gate="-43" pin="P" pad="43"/>
<connect gate="-44" pin="P" pad="44"/>
<connect gate="-45" pin="P" pad="45"/>
<connect gate="-46" pin="P" pad="46"/>
<connect gate="-47" pin="P" pad="47"/>
<connect gate="-48" pin="P" pad="48"/>
<connect gate="-49" pin="P" pad="49"/>
<connect gate="-5" pin="P" pad="5"/>
<connect gate="-50" pin="P" pad="50"/>
<connect gate="-51" pin="P" pad="51"/>
<connect gate="-52" pin="P" pad="52"/>
<connect gate="-53" pin="P" pad="53"/>
<connect gate="-54" pin="P" pad="54"/>
<connect gate="-55" pin="P" pad="55"/>
<connect gate="-56" pin="P" pad="56"/>
<connect gate="-57" pin="P" pad="57"/>
<connect gate="-58" pin="P" pad="58"/>
<connect gate="-59" pin="P" pad="59"/>
<connect gate="-6" pin="P" pad="6"/>
<connect gate="-60" pin="P" pad="60"/>
<connect gate="-61" pin="P" pad="61"/>
<connect gate="-62" pin="P" pad="62"/>
<connect gate="-63" pin="P" pad="63"/>
<connect gate="-64" pin="P" pad="64"/>
<connect gate="-65" pin="P" pad="65"/>
<connect gate="-66" pin="P" pad="66"/>
<connect gate="-67" pin="P" pad="67"/>
<connect gate="-68" pin="P" pad="68"/>
<connect gate="-69" pin="P" pad="69"/>
<connect gate="-7" pin="P" pad="7"/>
<connect gate="-70" pin="P" pad="70"/>
<connect gate="-71" pin="P" pad="71"/>
<connect gate="-72" pin="P" pad="72"/>
<connect gate="-73" pin="P" pad="73"/>
<connect gate="-74" pin="P" pad="74"/>
<connect gate="-75" pin="P" pad="75"/>
<connect gate="-76" pin="P" pad="76"/>
<connect gate="-77" pin="P" pad="77"/>
<connect gate="-78" pin="P" pad="78"/>
<connect gate="-79" pin="P" pad="79"/>
<connect gate="-8" pin="P" pad="8"/>
<connect gate="-80" pin="P" pad="80"/>
<connect gate="-81" pin="P" pad="81"/>
<connect gate="-82" pin="P" pad="82"/>
<connect gate="-83" pin="P" pad="83"/>
<connect gate="-84" pin="P" pad="84"/>
<connect gate="-85" pin="P" pad="85"/>
<connect gate="-86" pin="P" pad="86"/>
<connect gate="-87" pin="P" pad="87"/>
<connect gate="-88" pin="P" pad="88"/>
<connect gate="-89" pin="P" pad="89"/>
<connect gate="-9" pin="P" pad="9"/>
<connect gate="-90" pin="P" pad="90"/>
<connect gate="-91" pin="P" pad="91"/>
<connect gate="-92" pin="P" pad="92"/>
<connect gate="-93" pin="P" pad="93"/>
<connect gate="-94" pin="P" pad="94"/>
<connect gate="-95" pin="P" pad="95"/>
<connect gate="-96" pin="P" pad="96"/>
<connect gate="-97" pin="P" pad="97"/>
<connect gate="-98" pin="P" pad="98"/>
<connect gate="-99" pin="P" pad="99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AGP_UC-SLOT" prefix="X">
<description>&lt;b&gt;AGP:UC Slot&lt;/b&gt; AMP connctor 145376 &amp;gt;PCT-GF40&amp;lt; &lt;p&gt;
132 Position 1mm, card edge connector&lt;br&gt;
Drawing No: C-145263&lt;br&gt;
Source: http://ecommas.tycoelectronics.com .. ENG_CD_145376_D.pdf</description>
<gates>
<gate name="-1" symbol="MALEVAL"/>
<gate name="-2" symbol="MALEVAL"/>
<gate name="-3" symbol="MALE"/>
<gate name="-4" symbol="MALE"/>
<gate name="-5" symbol="MALE"/>
<gate name="-6" symbol="MALE"/>
<gate name="-7" symbol="MALE"/>
<gate name="-8" symbol="MALE"/>
<gate name="-9" symbol="MALE"/>
<gate name="-10" symbol="MALE"/>
<gate name="-11" symbol="MALE"/>
<gate name="-12" symbol="MALE"/>
<gate name="-13" symbol="MALE"/>
<gate name="-14" symbol="MALE"/>
<gate name="-15" symbol="MALE"/>
<gate name="-16" symbol="MALE"/>
<gate name="-17" symbol="MALE"/>
<gate name="-18" symbol="MALE"/>
<gate name="-19" symbol="MALE"/>
<gate name="-20" symbol="MALE"/>
<gate name="-21" symbol="MALE"/>
<gate name="-22" symbol="MALE"/>
<gate name="-23" symbol="MALE"/>
<gate name="-24" symbol="MALE"/>
<gate name="-25" symbol="MALE"/>
<gate name="-26" symbol="MALE"/>
<gate name="-27" symbol="MALE"/>
<gate name="-28" symbol="MALE"/>
<gate name="-29" symbol="MALE"/>
<gate name="-30" symbol="MALE"/>
<gate name="-31" symbol="MALE"/>
<gate name="-32" symbol="MALE"/>
<gate name="-33" symbol="MALE"/>
<gate name="-34" symbol="MALE"/>
<gate name="-35" symbol="MALE"/>
<gate name="-36" symbol="MALE"/>
<gate name="-37" symbol="MALE"/>
<gate name="-38" symbol="MALE"/>
<gate name="-39" symbol="MALE"/>
<gate name="-40" symbol="MALE"/>
<gate name="-41" symbol="MALE"/>
<gate name="-42" symbol="MALE"/>
<gate name="-43" symbol="MALE"/>
<gate name="-44" symbol="MALE"/>
<gate name="-45" symbol="MALE"/>
<gate name="-46" symbol="MALE"/>
<gate name="-47" symbol="MALE"/>
<gate name="-48" symbol="MALE"/>
<gate name="-49" symbol="MALE"/>
<gate name="-50" symbol="MALE"/>
<gate name="-51" symbol="MALE"/>
<gate name="-52" symbol="MALE"/>
<gate name="-53" symbol="MALE"/>
<gate name="-54" symbol="MALE"/>
<gate name="-55" symbol="MALE"/>
<gate name="-56" symbol="MALE"/>
<gate name="-57" symbol="MALE"/>
<gate name="-58" symbol="MALE"/>
<gate name="-59" symbol="MALE"/>
<gate name="-60" symbol="MALE"/>
<gate name="-61" symbol="MALE"/>
<gate name="-62" symbol="MALE"/>
<gate name="-63" symbol="MALE"/>
<gate name="-64" symbol="MALE"/>
<gate name="-65" symbol="MALE"/>
<gate name="-66" symbol="MALE"/>
<gate name="-67" symbol="MALE"/>
<gate name="-68" symbol="MALE"/>
<gate name="-69" symbol="MALE"/>
<gate name="-70" symbol="MALE"/>
<gate name="-71" symbol="MALE"/>
<gate name="-72" symbol="MALE"/>
<gate name="-73" symbol="MALE"/>
<gate name="-74" symbol="MALE"/>
<gate name="-75" symbol="MALE"/>
<gate name="-76" symbol="MALE"/>
<gate name="-77" symbol="MALE"/>
<gate name="-78" symbol="MALE"/>
<gate name="-79" symbol="MALE"/>
<gate name="-80" symbol="MALE"/>
<gate name="-81" symbol="MALE"/>
<gate name="-82" symbol="MALE"/>
<gate name="-83" symbol="MALE"/>
<gate name="-84" symbol="MALE"/>
<gate name="-85" symbol="MALE"/>
<gate name="-86" symbol="MALE"/>
<gate name="-87" symbol="MALE"/>
<gate name="-88" symbol="MALE"/>
<gate name="-89" symbol="MALE"/>
<gate name="-90" symbol="MALE"/>
<gate name="-91" symbol="MALE"/>
<gate name="-92" symbol="MALE"/>
<gate name="-93" symbol="MALE"/>
<gate name="-94" symbol="MALE"/>
<gate name="-95" symbol="MALE"/>
<gate name="-96" symbol="MALE"/>
<gate name="-97" symbol="MALE"/>
<gate name="-98" symbol="MALE"/>
<gate name="-99" symbol="MALE"/>
<gate name="-100" symbol="MALE"/>
<gate name="-101" symbol="MALE"/>
<gate name="-102" symbol="MALE"/>
<gate name="-103" symbol="MALE"/>
<gate name="-104" symbol="MALE"/>
<gate name="-105" symbol="MALE"/>
<gate name="-106" symbol="MALE"/>
<gate name="-107" symbol="MALE"/>
<gate name="-108" symbol="MALE"/>
<gate name="-109" symbol="MALE"/>
<gate name="-110" symbol="MALE"/>
<gate name="-111" symbol="MALE"/>
<gate name="-112" symbol="MALE"/>
<gate name="-113" symbol="MALE"/>
<gate name="-114" symbol="MALE"/>
<gate name="-115" symbol="MALE"/>
<gate name="-116" symbol="MALE"/>
<gate name="-117" symbol="MALE"/>
<gate name="-118" symbol="MALE"/>
<gate name="-119" symbol="MALE"/>
<gate name="-120" symbol="MALE"/>
<gate name="-121" symbol="MALE"/>
<gate name="-122" symbol="MALE"/>
<gate name="-123" symbol="MALE"/>
<gate name="-124" symbol="MALE"/>
<gate name="-125" symbol="MALE"/>
<gate name="-126" symbol="MALE"/>
<gate name="-127" symbol="MALE"/>
<gate name="-128" symbol="MALE"/>
<gate name="-129" symbol="MALE"/>
<gate name="-130" symbol="MALE"/>
<gate name="-131" symbol="MALE"/>
<gate name="-132" symbol="MALE"/>
</gates>
<devices>
<device name="" package="AGP_UC-SLOT">
<connects>
<connect gate="-1" pin="P" pad="1"/>
<connect gate="-10" pin="P" pad="10"/>
<connect gate="-100" pin="P" pad="100"/>
<connect gate="-101" pin="P" pad="101"/>
<connect gate="-102" pin="P" pad="102"/>
<connect gate="-103" pin="P" pad="103"/>
<connect gate="-104" pin="P" pad="104"/>
<connect gate="-105" pin="P" pad="105"/>
<connect gate="-106" pin="P" pad="106"/>
<connect gate="-107" pin="P" pad="107"/>
<connect gate="-108" pin="P" pad="108"/>
<connect gate="-109" pin="P" pad="109"/>
<connect gate="-11" pin="P" pad="11"/>
<connect gate="-110" pin="P" pad="110"/>
<connect gate="-111" pin="P" pad="111"/>
<connect gate="-112" pin="P" pad="112"/>
<connect gate="-113" pin="P" pad="113"/>
<connect gate="-114" pin="P" pad="114"/>
<connect gate="-115" pin="P" pad="115"/>
<connect gate="-116" pin="P" pad="116"/>
<connect gate="-117" pin="P" pad="117"/>
<connect gate="-118" pin="P" pad="118"/>
<connect gate="-119" pin="P" pad="119"/>
<connect gate="-12" pin="P" pad="12"/>
<connect gate="-120" pin="P" pad="120"/>
<connect gate="-121" pin="P" pad="121"/>
<connect gate="-122" pin="P" pad="122"/>
<connect gate="-123" pin="P" pad="123"/>
<connect gate="-124" pin="P" pad="124"/>
<connect gate="-125" pin="P" pad="125"/>
<connect gate="-126" pin="P" pad="126"/>
<connect gate="-127" pin="P" pad="127"/>
<connect gate="-128" pin="P" pad="128"/>
<connect gate="-129" pin="P" pad="129"/>
<connect gate="-13" pin="P" pad="13"/>
<connect gate="-130" pin="P" pad="130"/>
<connect gate="-131" pin="P" pad="131"/>
<connect gate="-132" pin="P" pad="132"/>
<connect gate="-14" pin="P" pad="14"/>
<connect gate="-15" pin="P" pad="15"/>
<connect gate="-16" pin="P" pad="16"/>
<connect gate="-17" pin="P" pad="17"/>
<connect gate="-18" pin="P" pad="18"/>
<connect gate="-19" pin="P" pad="19"/>
<connect gate="-2" pin="P" pad="2"/>
<connect gate="-20" pin="P" pad="20"/>
<connect gate="-21" pin="P" pad="21"/>
<connect gate="-22" pin="P" pad="22"/>
<connect gate="-23" pin="P" pad="23"/>
<connect gate="-24" pin="P" pad="24"/>
<connect gate="-25" pin="P" pad="25"/>
<connect gate="-26" pin="P" pad="26"/>
<connect gate="-27" pin="P" pad="27"/>
<connect gate="-28" pin="P" pad="28"/>
<connect gate="-29" pin="P" pad="29"/>
<connect gate="-3" pin="P" pad="3"/>
<connect gate="-30" pin="P" pad="30"/>
<connect gate="-31" pin="P" pad="31"/>
<connect gate="-32" pin="P" pad="32"/>
<connect gate="-33" pin="P" pad="33"/>
<connect gate="-34" pin="P" pad="34"/>
<connect gate="-35" pin="P" pad="35"/>
<connect gate="-36" pin="P" pad="36"/>
<connect gate="-37" pin="P" pad="37"/>
<connect gate="-38" pin="P" pad="38"/>
<connect gate="-39" pin="P" pad="39"/>
<connect gate="-4" pin="P" pad="4"/>
<connect gate="-40" pin="P" pad="40"/>
<connect gate="-41" pin="P" pad="41"/>
<connect gate="-42" pin="P" pad="42"/>
<connect gate="-43" pin="P" pad="43"/>
<connect gate="-44" pin="P" pad="44"/>
<connect gate="-45" pin="P" pad="45"/>
<connect gate="-46" pin="P" pad="46"/>
<connect gate="-47" pin="P" pad="47"/>
<connect gate="-48" pin="P" pad="48"/>
<connect gate="-49" pin="P" pad="49"/>
<connect gate="-5" pin="P" pad="5"/>
<connect gate="-50" pin="P" pad="50"/>
<connect gate="-51" pin="P" pad="51"/>
<connect gate="-52" pin="P" pad="52"/>
<connect gate="-53" pin="P" pad="53"/>
<connect gate="-54" pin="P" pad="54"/>
<connect gate="-55" pin="P" pad="55"/>
<connect gate="-56" pin="P" pad="56"/>
<connect gate="-57" pin="P" pad="57"/>
<connect gate="-58" pin="P" pad="58"/>
<connect gate="-59" pin="P" pad="59"/>
<connect gate="-6" pin="P" pad="6"/>
<connect gate="-60" pin="P" pad="60"/>
<connect gate="-61" pin="P" pad="61"/>
<connect gate="-62" pin="P" pad="62"/>
<connect gate="-63" pin="P" pad="63"/>
<connect gate="-64" pin="P" pad="64"/>
<connect gate="-65" pin="P" pad="65"/>
<connect gate="-66" pin="P" pad="66"/>
<connect gate="-67" pin="P" pad="67"/>
<connect gate="-68" pin="P" pad="68"/>
<connect gate="-69" pin="P" pad="69"/>
<connect gate="-7" pin="P" pad="7"/>
<connect gate="-70" pin="P" pad="70"/>
<connect gate="-71" pin="P" pad="71"/>
<connect gate="-72" pin="P" pad="72"/>
<connect gate="-73" pin="P" pad="73"/>
<connect gate="-74" pin="P" pad="74"/>
<connect gate="-75" pin="P" pad="75"/>
<connect gate="-76" pin="P" pad="76"/>
<connect gate="-77" pin="P" pad="77"/>
<connect gate="-78" pin="P" pad="78"/>
<connect gate="-79" pin="P" pad="79"/>
<connect gate="-8" pin="P" pad="8"/>
<connect gate="-80" pin="P" pad="80"/>
<connect gate="-81" pin="P" pad="81"/>
<connect gate="-82" pin="P" pad="82"/>
<connect gate="-83" pin="P" pad="83"/>
<connect gate="-84" pin="P" pad="84"/>
<connect gate="-85" pin="P" pad="85"/>
<connect gate="-86" pin="P" pad="86"/>
<connect gate="-87" pin="P" pad="87"/>
<connect gate="-88" pin="P" pad="88"/>
<connect gate="-89" pin="P" pad="89"/>
<connect gate="-9" pin="P" pad="9"/>
<connect gate="-90" pin="P" pad="90"/>
<connect gate="-91" pin="P" pad="91"/>
<connect gate="-92" pin="P" pad="92"/>
<connect gate="-93" pin="P" pad="93"/>
<connect gate="-94" pin="P" pad="94"/>
<connect gate="-95" pin="P" pad="95"/>
<connect gate="-96" pin="P" pad="96"/>
<connect gate="-97" pin="P" pad="97"/>
<connect gate="-98" pin="P" pad="98"/>
<connect gate="-99" pin="P" pad="99"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCI-E-164" prefix="X">
<description>Copy from  &lt;b&gt;con-pci_express(pci-e).lbr&lt;/b&gt; uploaded &lt;i&gt;Mon Jul 2 10:15:25 2007&lt;/i&gt;&lt;p&gt; 
Library for PCI-Express x16 (PCI-E) connector. Includes connector and card edge pattern.&lt;br&gt;
Uploaded by JF Duval &amp;lt;jfduval@aqra.ca&amp;gt; from AQRA.ca</description>
<gates>
<gate name="G$1" symbol="PCI-E-164"/>
</gates>
<devices>
<device name="SLOT" package="PCI-E_SLOT">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A16" pad="A16"/>
<connect gate="G$1" pin="A17" pad="A17"/>
<connect gate="G$1" pin="A18" pad="A18"/>
<connect gate="G$1" pin="A19" pad="A19"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A20" pad="A20"/>
<connect gate="G$1" pin="A21" pad="A21"/>
<connect gate="G$1" pin="A22" pad="A22"/>
<connect gate="G$1" pin="A23" pad="A23"/>
<connect gate="G$1" pin="A24" pad="A24"/>
<connect gate="G$1" pin="A25" pad="A25"/>
<connect gate="G$1" pin="A26" pad="A26"/>
<connect gate="G$1" pin="A27" pad="A27"/>
<connect gate="G$1" pin="A28" pad="A28"/>
<connect gate="G$1" pin="A29" pad="A29"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A30" pad="A30"/>
<connect gate="G$1" pin="A31" pad="A31"/>
<connect gate="G$1" pin="A32" pad="A32"/>
<connect gate="G$1" pin="A33" pad="A33"/>
<connect gate="G$1" pin="A34" pad="A34"/>
<connect gate="G$1" pin="A35" pad="A35"/>
<connect gate="G$1" pin="A36" pad="A36"/>
<connect gate="G$1" pin="A37" pad="A37"/>
<connect gate="G$1" pin="A38" pad="A38"/>
<connect gate="G$1" pin="A39" pad="A39"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A40" pad="A40"/>
<connect gate="G$1" pin="A41" pad="A41"/>
<connect gate="G$1" pin="A42" pad="A42"/>
<connect gate="G$1" pin="A43" pad="A43"/>
<connect gate="G$1" pin="A44" pad="A44"/>
<connect gate="G$1" pin="A45" pad="A45"/>
<connect gate="G$1" pin="A46" pad="A46"/>
<connect gate="G$1" pin="A47" pad="A47"/>
<connect gate="G$1" pin="A48" pad="A48"/>
<connect gate="G$1" pin="A49" pad="A49"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A50" pad="A50"/>
<connect gate="G$1" pin="A51" pad="A51"/>
<connect gate="G$1" pin="A52" pad="A52"/>
<connect gate="G$1" pin="A53" pad="A53"/>
<connect gate="G$1" pin="A54" pad="A54"/>
<connect gate="G$1" pin="A55" pad="A55"/>
<connect gate="G$1" pin="A56" pad="A56"/>
<connect gate="G$1" pin="A57" pad="A57"/>
<connect gate="G$1" pin="A58" pad="A58"/>
<connect gate="G$1" pin="A59" pad="A59"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A60" pad="A60"/>
<connect gate="G$1" pin="A61" pad="A61"/>
<connect gate="G$1" pin="A62" pad="A62"/>
<connect gate="G$1" pin="A63" pad="A63"/>
<connect gate="G$1" pin="A64" pad="A64"/>
<connect gate="G$1" pin="A65" pad="A65"/>
<connect gate="G$1" pin="A66" pad="A66"/>
<connect gate="G$1" pin="A67" pad="A67"/>
<connect gate="G$1" pin="A68" pad="A68"/>
<connect gate="G$1" pin="A69" pad="A69"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A70" pad="A70"/>
<connect gate="G$1" pin="A71" pad="A71"/>
<connect gate="G$1" pin="A72" pad="A72"/>
<connect gate="G$1" pin="A73" pad="A73"/>
<connect gate="G$1" pin="A74" pad="A74"/>
<connect gate="G$1" pin="A75" pad="A75"/>
<connect gate="G$1" pin="A76" pad="A76"/>
<connect gate="G$1" pin="A77" pad="A77"/>
<connect gate="G$1" pin="A78" pad="A78"/>
<connect gate="G$1" pin="A79" pad="A79"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A80" pad="A80"/>
<connect gate="G$1" pin="A81" pad="A81"/>
<connect gate="G$1" pin="A82" pad="A82"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B13" pad="B13"/>
<connect gate="G$1" pin="B14" pad="B14"/>
<connect gate="G$1" pin="B15" pad="B15"/>
<connect gate="G$1" pin="B16" pad="B16"/>
<connect gate="G$1" pin="B17" pad="B17"/>
<connect gate="G$1" pin="B18" pad="B18"/>
<connect gate="G$1" pin="B19" pad="B19"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B20" pad="B20"/>
<connect gate="G$1" pin="B21" pad="B21"/>
<connect gate="G$1" pin="B22" pad="B22"/>
<connect gate="G$1" pin="B23" pad="B23"/>
<connect gate="G$1" pin="B24" pad="B24"/>
<connect gate="G$1" pin="B25" pad="B25"/>
<connect gate="G$1" pin="B26" pad="B26"/>
<connect gate="G$1" pin="B27" pad="B27"/>
<connect gate="G$1" pin="B28" pad="B28"/>
<connect gate="G$1" pin="B29" pad="B29"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B30" pad="B30"/>
<connect gate="G$1" pin="B31" pad="B31"/>
<connect gate="G$1" pin="B32" pad="B32"/>
<connect gate="G$1" pin="B33" pad="B33"/>
<connect gate="G$1" pin="B34" pad="B34"/>
<connect gate="G$1" pin="B35" pad="B35"/>
<connect gate="G$1" pin="B36" pad="B36"/>
<connect gate="G$1" pin="B37" pad="B37"/>
<connect gate="G$1" pin="B38" pad="B38"/>
<connect gate="G$1" pin="B39" pad="B39"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B40" pad="B40"/>
<connect gate="G$1" pin="B41" pad="B41"/>
<connect gate="G$1" pin="B42" pad="B42"/>
<connect gate="G$1" pin="B43" pad="B43"/>
<connect gate="G$1" pin="B44" pad="B44"/>
<connect gate="G$1" pin="B45" pad="B45"/>
<connect gate="G$1" pin="B46" pad="B46"/>
<connect gate="G$1" pin="B47" pad="B47"/>
<connect gate="G$1" pin="B48" pad="B48"/>
<connect gate="G$1" pin="B49" pad="B49"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B50" pad="B50"/>
<connect gate="G$1" pin="B51" pad="B51"/>
<connect gate="G$1" pin="B52" pad="B52"/>
<connect gate="G$1" pin="B53" pad="B53"/>
<connect gate="G$1" pin="B54" pad="B54"/>
<connect gate="G$1" pin="B55" pad="B55"/>
<connect gate="G$1" pin="B56" pad="B56"/>
<connect gate="G$1" pin="B57" pad="B57"/>
<connect gate="G$1" pin="B58" pad="B58"/>
<connect gate="G$1" pin="B59" pad="B59"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B60" pad="B60"/>
<connect gate="G$1" pin="B61" pad="B61"/>
<connect gate="G$1" pin="B62" pad="B62"/>
<connect gate="G$1" pin="B63" pad="B63"/>
<connect gate="G$1" pin="B64" pad="B64"/>
<connect gate="G$1" pin="B65" pad="B65"/>
<connect gate="G$1" pin="B66" pad="B66"/>
<connect gate="G$1" pin="B67" pad="B67"/>
<connect gate="G$1" pin="B68" pad="B68"/>
<connect gate="G$1" pin="B69" pad="B69"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B70" pad="B70"/>
<connect gate="G$1" pin="B71" pad="B71"/>
<connect gate="G$1" pin="B72" pad="B72"/>
<connect gate="G$1" pin="B73" pad="B73"/>
<connect gate="G$1" pin="B74" pad="B74"/>
<connect gate="G$1" pin="B75" pad="B75"/>
<connect gate="G$1" pin="B76" pad="B76"/>
<connect gate="G$1" pin="B77" pad="B77"/>
<connect gate="G$1" pin="B78" pad="B78"/>
<connect gate="G$1" pin="B79" pad="B79"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B80" pad="B80"/>
<connect gate="G$1" pin="B81" pad="B81"/>
<connect gate="G$1" pin="B82" pad="B82"/>
<connect gate="G$1" pin="B9" pad="B9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOCKET" package="PCI-E-164">
<connects>
<connect gate="G$1" pin="A1" pad="A1"/>
<connect gate="G$1" pin="A10" pad="A10"/>
<connect gate="G$1" pin="A11" pad="A11"/>
<connect gate="G$1" pin="A12" pad="A12"/>
<connect gate="G$1" pin="A13" pad="A13"/>
<connect gate="G$1" pin="A14" pad="A14"/>
<connect gate="G$1" pin="A15" pad="A15"/>
<connect gate="G$1" pin="A16" pad="A16"/>
<connect gate="G$1" pin="A17" pad="A17"/>
<connect gate="G$1" pin="A18" pad="A18"/>
<connect gate="G$1" pin="A19" pad="A19"/>
<connect gate="G$1" pin="A2" pad="A2"/>
<connect gate="G$1" pin="A20" pad="A20"/>
<connect gate="G$1" pin="A21" pad="A21"/>
<connect gate="G$1" pin="A22" pad="A22"/>
<connect gate="G$1" pin="A23" pad="A23"/>
<connect gate="G$1" pin="A24" pad="A24"/>
<connect gate="G$1" pin="A25" pad="A25"/>
<connect gate="G$1" pin="A26" pad="A26"/>
<connect gate="G$1" pin="A27" pad="A27"/>
<connect gate="G$1" pin="A28" pad="A28"/>
<connect gate="G$1" pin="A29" pad="A29"/>
<connect gate="G$1" pin="A3" pad="A3"/>
<connect gate="G$1" pin="A30" pad="A30"/>
<connect gate="G$1" pin="A31" pad="A31"/>
<connect gate="G$1" pin="A32" pad="A32"/>
<connect gate="G$1" pin="A33" pad="A33"/>
<connect gate="G$1" pin="A34" pad="A34"/>
<connect gate="G$1" pin="A35" pad="A35"/>
<connect gate="G$1" pin="A36" pad="A36"/>
<connect gate="G$1" pin="A37" pad="A37"/>
<connect gate="G$1" pin="A38" pad="A38"/>
<connect gate="G$1" pin="A39" pad="A39"/>
<connect gate="G$1" pin="A4" pad="A4"/>
<connect gate="G$1" pin="A40" pad="A40"/>
<connect gate="G$1" pin="A41" pad="A41"/>
<connect gate="G$1" pin="A42" pad="A42"/>
<connect gate="G$1" pin="A43" pad="A43"/>
<connect gate="G$1" pin="A44" pad="A44"/>
<connect gate="G$1" pin="A45" pad="A45"/>
<connect gate="G$1" pin="A46" pad="A46"/>
<connect gate="G$1" pin="A47" pad="A47"/>
<connect gate="G$1" pin="A48" pad="A48"/>
<connect gate="G$1" pin="A49" pad="A49"/>
<connect gate="G$1" pin="A5" pad="A5"/>
<connect gate="G$1" pin="A50" pad="A50"/>
<connect gate="G$1" pin="A51" pad="A51"/>
<connect gate="G$1" pin="A52" pad="A52"/>
<connect gate="G$1" pin="A53" pad="A53"/>
<connect gate="G$1" pin="A54" pad="A54"/>
<connect gate="G$1" pin="A55" pad="A55"/>
<connect gate="G$1" pin="A56" pad="A56"/>
<connect gate="G$1" pin="A57" pad="A57"/>
<connect gate="G$1" pin="A58" pad="A58"/>
<connect gate="G$1" pin="A59" pad="A59"/>
<connect gate="G$1" pin="A6" pad="A6"/>
<connect gate="G$1" pin="A60" pad="A60"/>
<connect gate="G$1" pin="A61" pad="A61"/>
<connect gate="G$1" pin="A62" pad="A62"/>
<connect gate="G$1" pin="A63" pad="A63"/>
<connect gate="G$1" pin="A64" pad="A64"/>
<connect gate="G$1" pin="A65" pad="A65"/>
<connect gate="G$1" pin="A66" pad="A66"/>
<connect gate="G$1" pin="A67" pad="A67"/>
<connect gate="G$1" pin="A68" pad="A68"/>
<connect gate="G$1" pin="A69" pad="A69"/>
<connect gate="G$1" pin="A7" pad="A7"/>
<connect gate="G$1" pin="A70" pad="A70"/>
<connect gate="G$1" pin="A71" pad="A71"/>
<connect gate="G$1" pin="A72" pad="A72"/>
<connect gate="G$1" pin="A73" pad="A73"/>
<connect gate="G$1" pin="A74" pad="A74"/>
<connect gate="G$1" pin="A75" pad="A75"/>
<connect gate="G$1" pin="A76" pad="A76"/>
<connect gate="G$1" pin="A77" pad="A77"/>
<connect gate="G$1" pin="A78" pad="A78"/>
<connect gate="G$1" pin="A79" pad="A79"/>
<connect gate="G$1" pin="A8" pad="A8"/>
<connect gate="G$1" pin="A80" pad="A80"/>
<connect gate="G$1" pin="A81" pad="A81"/>
<connect gate="G$1" pin="A82" pad="A82"/>
<connect gate="G$1" pin="A9" pad="A9"/>
<connect gate="G$1" pin="B1" pad="B1"/>
<connect gate="G$1" pin="B10" pad="B10"/>
<connect gate="G$1" pin="B11" pad="B11"/>
<connect gate="G$1" pin="B12" pad="B12"/>
<connect gate="G$1" pin="B13" pad="B13"/>
<connect gate="G$1" pin="B14" pad="B14"/>
<connect gate="G$1" pin="B15" pad="B15"/>
<connect gate="G$1" pin="B16" pad="B16"/>
<connect gate="G$1" pin="B17" pad="B17"/>
<connect gate="G$1" pin="B18" pad="B18"/>
<connect gate="G$1" pin="B19" pad="B19"/>
<connect gate="G$1" pin="B2" pad="B2"/>
<connect gate="G$1" pin="B20" pad="B20"/>
<connect gate="G$1" pin="B21" pad="B21"/>
<connect gate="G$1" pin="B22" pad="B22"/>
<connect gate="G$1" pin="B23" pad="B23"/>
<connect gate="G$1" pin="B24" pad="B24"/>
<connect gate="G$1" pin="B25" pad="B25"/>
<connect gate="G$1" pin="B26" pad="B26"/>
<connect gate="G$1" pin="B27" pad="B27"/>
<connect gate="G$1" pin="B28" pad="B28"/>
<connect gate="G$1" pin="B29" pad="B29"/>
<connect gate="G$1" pin="B3" pad="B3"/>
<connect gate="G$1" pin="B30" pad="B30"/>
<connect gate="G$1" pin="B31" pad="B31"/>
<connect gate="G$1" pin="B32" pad="B32"/>
<connect gate="G$1" pin="B33" pad="B33"/>
<connect gate="G$1" pin="B34" pad="B34"/>
<connect gate="G$1" pin="B35" pad="B35"/>
<connect gate="G$1" pin="B36" pad="B36"/>
<connect gate="G$1" pin="B37" pad="B37"/>
<connect gate="G$1" pin="B38" pad="B38"/>
<connect gate="G$1" pin="B39" pad="B39"/>
<connect gate="G$1" pin="B4" pad="B4"/>
<connect gate="G$1" pin="B40" pad="B40"/>
<connect gate="G$1" pin="B41" pad="B41"/>
<connect gate="G$1" pin="B42" pad="B42"/>
<connect gate="G$1" pin="B43" pad="B43"/>
<connect gate="G$1" pin="B44" pad="B44"/>
<connect gate="G$1" pin="B45" pad="B45"/>
<connect gate="G$1" pin="B46" pad="B46"/>
<connect gate="G$1" pin="B47" pad="B47"/>
<connect gate="G$1" pin="B48" pad="B48"/>
<connect gate="G$1" pin="B49" pad="B49"/>
<connect gate="G$1" pin="B5" pad="B5"/>
<connect gate="G$1" pin="B50" pad="B50"/>
<connect gate="G$1" pin="B51" pad="B51"/>
<connect gate="G$1" pin="B52" pad="B52"/>
<connect gate="G$1" pin="B53" pad="B53"/>
<connect gate="G$1" pin="B54" pad="B54"/>
<connect gate="G$1" pin="B55" pad="B55"/>
<connect gate="G$1" pin="B56" pad="B56"/>
<connect gate="G$1" pin="B57" pad="B57"/>
<connect gate="G$1" pin="B58" pad="B58"/>
<connect gate="G$1" pin="B59" pad="B59"/>
<connect gate="G$1" pin="B6" pad="B6"/>
<connect gate="G$1" pin="B60" pad="B60"/>
<connect gate="G$1" pin="B61" pad="B61"/>
<connect gate="G$1" pin="B62" pad="B62"/>
<connect gate="G$1" pin="B63" pad="B63"/>
<connect gate="G$1" pin="B64" pad="B64"/>
<connect gate="G$1" pin="B65" pad="B65"/>
<connect gate="G$1" pin="B66" pad="B66"/>
<connect gate="G$1" pin="B67" pad="B67"/>
<connect gate="G$1" pin="B68" pad="B68"/>
<connect gate="G$1" pin="B69" pad="B69"/>
<connect gate="G$1" pin="B7" pad="B7"/>
<connect gate="G$1" pin="B70" pad="B70"/>
<connect gate="G$1" pin="B71" pad="B71"/>
<connect gate="G$1" pin="B72" pad="B72"/>
<connect gate="G$1" pin="B73" pad="B73"/>
<connect gate="G$1" pin="B74" pad="B74"/>
<connect gate="G$1" pin="B75" pad="B75"/>
<connect gate="G$1" pin="B76" pad="B76"/>
<connect gate="G$1" pin="B77" pad="B77"/>
<connect gate="G$1" pin="B78" pad="B78"/>
<connect gate="G$1" pin="B79" pad="B79"/>
<connect gate="G$1" pin="B8" pad="B8"/>
<connect gate="G$1" pin="B80" pad="B80"/>
<connect gate="G$1" pin="B81" pad="B81"/>
<connect gate="G$1" pin="B82" pad="B82"/>
<connect gate="G$1" pin="B9" pad="B9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
