<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.2">
<drawing>
<library>
<description>&lt;b&gt;KINGBRIGHT Numeric Displays&lt;/b&gt;&lt;p&gt;
&lt;author&gt;librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SA56-11">
<description>&lt;b&gt;Kingbright 14.2mm (0.56 INCH) SINGLE DIGIT NUMERIC DUISPLAY&lt;/b&gt;&lt;p&gt;
Source: SA56-11EWA(Ver1189471036.pdf</description>
</package>
<package name="SA10-21">
<description>&lt;b&gt;25.4mm (1.0 INCH) SINGLE DIGIT NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;
Source: SA10-21EWA(Ver1189472078.10).pdf&lt;br&gt;
&lt;a href="http://www.farnell.com/datasheets/57132.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="SA18-11">
<description>&lt;b&gt;44.5mm (1.75INCH) SINGLE DIGIT NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;
Source: SA18-11EWA(Ver1189472866.5).pdf&lt;br&gt;
&lt;a href="http://www.farnell.com/datasheets/58023.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="PSA12-11">
<description>&lt;b&gt;30.48mm(1.2 INCH) 16 SEGMENT SINGLE DIGIT ALPHANUMERIC NUMERIC DISPLAY&lt;/b&gt;
Source: PSA12-11EWA(Ver1189413040.8).pdf</description>
</package>
<package name="SA52-11">
<description>&lt;b&gt;13.2mm (0.52INCH) SINGLE DIGIT NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/SA52-11EWA(Ver1195708215.10)</description>
</package>
<package name="SA39-11SRWA">
</package>
<package name="BA/BC56">
<description>&lt;b&gt;14.22mm (0.56INCH) THREE DIGIT NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com .. BA56-11EWA(Ver1189474895.pdf</description>
</package>
<package name="DA56">
<description>&lt;b&gt;14.22mm (0.56INCH) DUAL DIGIT NUMERIC DISPLAYS&lt;/b&gt;&lt;p&gt;
Source: DA56-11SRWA.pdf</description>
</package>
<package name="BX56-12">
<description>&lt;b&gt;14.22mm (0.56INCH) THREE DIGIT NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com .. BA56-11EWA(Ver1189474895.pdf</description>
</package>
<package name="TA20-11HWA">
<description>&lt;b&gt;50mm (2.0 INCH) 5x7 DOT MATRIX DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/TC20-11EWA(Ver1189410378.9)</description>
</package>
</packages>
<symbols>
<symbol name="7SEG-LED-COM2">
<pin name="DP" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="COM@1" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="COM@2" direction="pas"/>
</symbol>
<symbol name="16-SEG-LED-A">
<pin name="A" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="H" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="M" direction="pas"/>
<pin name="N" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="R" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="T" direction="pas"/>
<pin name="U" direction="pas"/>
<pin name="DP" direction="pas"/>
<pin name="AN" direction="pas"/>
</symbol>
<symbol name="7SEG-LED-COM1">
<pin name="DP" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="COM" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="7SEG-3-COM">
<pin name="DP" direction="pas"/>
<pin name="F" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="CA@3" direction="pas"/>
<pin name="C" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="CA@2" direction="pas"/>
<pin name="CA@1" direction="pas"/>
</symbol>
<symbol name="DOTMATIX-35A">
<pin name="R1" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="R3" direction="pas"/>
<pin name="R4" direction="pas"/>
<pin name="R5" direction="pas"/>
<pin name="R6" direction="pas"/>
<pin name="R7" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="C5" direction="pas"/>
<pin name="R4@1" direction="pas"/>
<pin name="C3@1" direction="pas"/>
</symbol>
<symbol name="DOTMATIX-35C">
<pin name="R1" direction="pas"/>
<pin name="R2" direction="pas"/>
<pin name="R3" direction="pas"/>
<pin name="R4" direction="pas"/>
<pin name="R5" direction="pas"/>
<pin name="R6" direction="pas"/>
<pin name="R7" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="C2" direction="pas"/>
<pin name="C3" direction="pas"/>
<pin name="C4" direction="pas"/>
<pin name="C5" direction="pas"/>
<pin name="R4@1" direction="pas"/>
<pin name="C3@1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="7-SEG_" prefix="LED">
<description>&lt;b&gt;Kingbright 14.2mm (0.56 INCH) SINGLE DIGIT NUMERIC DUISPLAY&lt;/b&gt;&lt;p&gt;
Source: SA56-11EWA(Ver1189471036.pdf</description>
<gates>
<gate name="G$1" symbol="7SEG-LED-COM2"/>
</gates>
<devices>
<device name="SA56-11" package="SA56-11">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="COM@1" pad="3"/>
<connect gate="G$1" pin="COM@2" pad="8"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SA10-21" package="SA10-21">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="COM@1" pad="3"/>
<connect gate="G$1" pin="COM@2" pad="8"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SA18-11" package="SA18-11">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="COM@1" pad="1"/>
<connect gate="G$1" pin="COM@2" pad="5"/>
<connect gate="G$1" pin="D" pad="3"/>
<connect gate="G$1" pin="DP" pad="8"/>
<connect gate="G$1" pin="E" pad="2"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SA52-11" package="SA52-11">
<connects>
<connect gate="G$1" pin="A" pad="7"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="G$1" pin="COM@1" pad="3"/>
<connect gate="G$1" pin="COM@2" pad="8"/>
<connect gate="G$1" pin="D" pad="2"/>
<connect gate="G$1" pin="DP" pad="5"/>
<connect gate="G$1" pin="E" pad="1"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SA39-11SRWA" package="SA39-11SRWA">
<connects>
<connect gate="G$1" pin="A" pad="10"/>
<connect gate="G$1" pin="B" pad="9"/>
<connect gate="G$1" pin="C" pad="7"/>
<connect gate="G$1" pin="COM@1" pad="3"/>
<connect gate="G$1" pin="COM@2" pad="8"/>
<connect gate="G$1" pin="D" pad="5"/>
<connect gate="G$1" pin="DP" pad="6"/>
<connect gate="G$1" pin="E" pad="4"/>
<connect gate="G$1" pin="F" pad="2"/>
<connect gate="G$1" pin="G" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="16-SEG_" prefix="LED">
<description>&lt;b&gt;16 SEGMENT SINGLE DIGIT ALPHANUMERIC NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="16-SEG-LED-A"/>
</gates>
<devices>
<device name="PSA12-11" package="PSA12-11">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="AN" pad="11"/>
<connect gate="G$1" pin="B" pad="18"/>
<connect gate="G$1" pin="C" pad="16"/>
<connect gate="G$1" pin="D" pad="13"/>
<connect gate="G$1" pin="DP" pad="12"/>
<connect gate="G$1" pin="E" pad="10"/>
<connect gate="G$1" pin="F" pad="9"/>
<connect gate="G$1" pin="G" pad="8"/>
<connect gate="G$1" pin="H" pad="4"/>
<connect gate="G$1" pin="K" pad="3"/>
<connect gate="G$1" pin="M" pad="2"/>
<connect gate="G$1" pin="N" pad="17"/>
<connect gate="G$1" pin="P" pad="15"/>
<connect gate="G$1" pin="R" pad="14"/>
<connect gate="G$1" pin="S" pad="6"/>
<connect gate="G$1" pin="T" pad="7"/>
<connect gate="G$1" pin="U" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="B?56-11*WA" prefix="LED">
<description>&lt;b&gt;14.22mm (0.56INCH) THREE DIGIT NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com .. BA56-11EWA(Ver1189474895.pdf</description>
<gates>
<gate name="DIG2" symbol="7SEG-LED-COM1"/>
<gate name="DIG3" symbol="7SEG-LED-COM1"/>
<gate name="DIG1" symbol="7SEG-LED-COM2"/>
</gates>
<devices>
<device name="A" package="BA/BC56">
<connects>
<connect gate="DIG1" pin="A" pad="25"/>
<connect gate="DIG1" pin="B" pad="24"/>
<connect gate="DIG1" pin="C" pad="4"/>
<connect gate="DIG1" pin="COM@1" pad="3"/>
<connect gate="DIG1" pin="COM@2" pad="26"/>
<connect gate="DIG1" pin="D" pad="2"/>
<connect gate="DIG1" pin="DP" pad="5"/>
<connect gate="DIG1" pin="E" pad="1"/>
<connect gate="DIG1" pin="F" pad="27"/>
<connect gate="DIG1" pin="G" pad="28"/>
<connect gate="DIG2" pin="A" pad="21"/>
<connect gate="DIG2" pin="B" pad="20"/>
<connect gate="DIG2" pin="C" pad="8"/>
<connect gate="DIG2" pin="COM" pad="19"/>
<connect gate="DIG2" pin="D" pad="7"/>
<connect gate="DIG2" pin="DP" pad="9"/>
<connect gate="DIG2" pin="E" pad="6"/>
<connect gate="DIG2" pin="F" pad="23"/>
<connect gate="DIG2" pin="G" pad="22"/>
<connect gate="DIG3" pin="A" pad="16"/>
<connect gate="DIG3" pin="B" pad="15"/>
<connect gate="DIG3" pin="C" pad="13"/>
<connect gate="DIG3" pin="COM" pad="18"/>
<connect gate="DIG3" pin="D" pad="11"/>
<connect gate="DIG3" pin="DP" pad="14"/>
<connect gate="DIG3" pin="E" pad="10"/>
<connect gate="DIG3" pin="F" pad="17"/>
<connect gate="DIG3" pin="G" pad="12"/>
</connects>
<technologies>
<technology name="E">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="G">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="SR">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Y">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="C" package="BA/BC56">
<connects>
<connect gate="DIG1" pin="A" pad="25"/>
<connect gate="DIG1" pin="B" pad="24"/>
<connect gate="DIG1" pin="C" pad="4"/>
<connect gate="DIG1" pin="COM@1" pad="3"/>
<connect gate="DIG1" pin="COM@2" pad="26"/>
<connect gate="DIG1" pin="D" pad="2"/>
<connect gate="DIG1" pin="DP" pad="5"/>
<connect gate="DIG1" pin="E" pad="1"/>
<connect gate="DIG1" pin="F" pad="27"/>
<connect gate="DIG1" pin="G" pad="28"/>
<connect gate="DIG2" pin="A" pad="21"/>
<connect gate="DIG2" pin="B" pad="20"/>
<connect gate="DIG2" pin="C" pad="8"/>
<connect gate="DIG2" pin="COM" pad="19"/>
<connect gate="DIG2" pin="D" pad="7"/>
<connect gate="DIG2" pin="DP" pad="9"/>
<connect gate="DIG2" pin="E" pad="6"/>
<connect gate="DIG2" pin="F" pad="23"/>
<connect gate="DIG2" pin="G" pad="22"/>
<connect gate="DIG3" pin="A" pad="16"/>
<connect gate="DIG3" pin="B" pad="15"/>
<connect gate="DIG3" pin="C" pad="13"/>
<connect gate="DIG3" pin="COM" pad="18"/>
<connect gate="DIG3" pin="D" pad="11"/>
<connect gate="DIG3" pin="DP" pad="14"/>
<connect gate="DIG3" pin="E" pad="10"/>
<connect gate="DIG3" pin="F" pad="17"/>
<connect gate="DIG3" pin="G" pad="12"/>
</connects>
<technologies>
<technology name="E">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="G">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="SR">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Y">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DA56-11" prefix="LED">
<description>&lt;b&gt;14.22mm (0.56INCH) DUAL DIGIT NUMERIC DISPLAYS&lt;/b&gt;&lt;p&gt;
Source: www.kingbright.com .. DA56-11SRWA.pdf</description>
<gates>
<gate name="DIG1" symbol="7SEG-LED-COM1"/>
<gate name="DIG2" symbol="7SEG-LED-COM1"/>
</gates>
<devices>
<device name="" package="DA56">
<connects>
<connect gate="DIG1" pin="A" pad="16"/>
<connect gate="DIG1" pin="B" pad="15"/>
<connect gate="DIG1" pin="C" pad="3"/>
<connect gate="DIG1" pin="COM" pad="14"/>
<connect gate="DIG1" pin="D" pad="2"/>
<connect gate="DIG1" pin="DP" pad="4"/>
<connect gate="DIG1" pin="E" pad="1"/>
<connect gate="DIG1" pin="F" pad="18"/>
<connect gate="DIG1" pin="G" pad="17"/>
<connect gate="DIG2" pin="A" pad="11"/>
<connect gate="DIG2" pin="B" pad="10"/>
<connect gate="DIG2" pin="C" pad="8"/>
<connect gate="DIG2" pin="COM" pad="13"/>
<connect gate="DIG2" pin="D" pad="6"/>
<connect gate="DIG2" pin="DP" pad="9"/>
<connect gate="DIG2" pin="E" pad="5"/>
<connect gate="DIG2" pin="F" pad="12"/>
<connect gate="DIG2" pin="G" pad="7"/>
</connects>
<technologies>
<technology name="EWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="GWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="SRWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="YWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DC56-11" prefix="LED">
<description>&lt;b&gt;14.22mm (0.56INCH) DUAL DIGIT NUMERIC DISPLAYS&lt;/b&gt;&lt;p&gt;
Source: www.kingbright.com .. DA56-11SRWA.pdf</description>
<gates>
<gate name="DIG1" symbol="7SEG-LED-COM1"/>
<gate name="DIG2" symbol="7SEG-LED-COM1"/>
</gates>
<devices>
<device name="" package="DA56">
<connects>
<connect gate="DIG1" pin="A" pad="16"/>
<connect gate="DIG1" pin="B" pad="15"/>
<connect gate="DIG1" pin="C" pad="3"/>
<connect gate="DIG1" pin="COM" pad="14"/>
<connect gate="DIG1" pin="D" pad="2"/>
<connect gate="DIG1" pin="DP" pad="4"/>
<connect gate="DIG1" pin="E" pad="1"/>
<connect gate="DIG1" pin="F" pad="18"/>
<connect gate="DIG1" pin="G" pad="17"/>
<connect gate="DIG2" pin="A" pad="11"/>
<connect gate="DIG2" pin="B" pad="10"/>
<connect gate="DIG2" pin="C" pad="8"/>
<connect gate="DIG2" pin="COM" pad="13"/>
<connect gate="DIG2" pin="D" pad="6"/>
<connect gate="DIG2" pin="DP" pad="9"/>
<connect gate="DIG2" pin="E" pad="5"/>
<connect gate="DIG2" pin="F" pad="12"/>
<connect gate="DIG2" pin="G" pad="7"/>
</connects>
<technologies>
<technology name="EWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="GWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="SRWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="YWA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="B?56-13*WA" prefix="LED">
<description>&lt;b&gt;14.22mm (0.56INCH) THREE DIGIT NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com .. BA56-11EWA(Ver1189474895.pdf</description>
<gates>
<gate name="DIG1" symbol="7SEG-LED-COM1"/>
<gate name="DIG2" symbol="7SEG-LED-COM2"/>
<gate name="DIG3" symbol="7SEG-LED-COM1"/>
</gates>
<devices>
<device name="A" package="BA/BC56">
<connects>
<connect gate="DIG1" pin="A" pad="27"/>
<connect gate="DIG1" pin="B" pad="24"/>
<connect gate="DIG1" pin="C" pad="3"/>
<connect gate="DIG1" pin="COM" pad="26"/>
<connect gate="DIG1" pin="D" pad="2"/>
<connect gate="DIG1" pin="DP" pad="4"/>
<connect gate="DIG1" pin="E" pad="1"/>
<connect gate="DIG1" pin="F" pad="28"/>
<connect gate="DIG1" pin="G" pad="25"/>
<connect gate="DIG2" pin="A" pad="22"/>
<connect gate="DIG2" pin="B" pad="19"/>
<connect gate="DIG2" pin="C" pad="7"/>
<connect gate="DIG2" pin="COM@1" pad="8"/>
<connect gate="DIG2" pin="COM@2" pad="21"/>
<connect gate="DIG2" pin="D" pad="6"/>
<connect gate="DIG2" pin="DP" pad="9"/>
<connect gate="DIG2" pin="E" pad="5"/>
<connect gate="DIG2" pin="F" pad="23"/>
<connect gate="DIG2" pin="G" pad="20"/>
<connect gate="DIG3" pin="A" pad="16"/>
<connect gate="DIG3" pin="B" pad="14"/>
<connect gate="DIG3" pin="C" pad="12"/>
<connect gate="DIG3" pin="COM" pad="15"/>
<connect gate="DIG3" pin="D" pad="11"/>
<connect gate="DIG3" pin="DP" pad="13"/>
<connect gate="DIG3" pin="E" pad="10"/>
<connect gate="DIG3" pin="F" pad="17"/>
<connect gate="DIG3" pin="G" pad="18"/>
</connects>
<technologies>
<technology name="E">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="G">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="SR">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Y">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="C" package="BA/BC56">
<connects>
<connect gate="DIG1" pin="A" pad="27"/>
<connect gate="DIG1" pin="B" pad="24"/>
<connect gate="DIG1" pin="C" pad="3"/>
<connect gate="DIG1" pin="COM" pad="26"/>
<connect gate="DIG1" pin="D" pad="2"/>
<connect gate="DIG1" pin="DP" pad="4"/>
<connect gate="DIG1" pin="E" pad="1"/>
<connect gate="DIG1" pin="F" pad="28"/>
<connect gate="DIG1" pin="G" pad="25"/>
<connect gate="DIG2" pin="A" pad="22"/>
<connect gate="DIG2" pin="B" pad="19"/>
<connect gate="DIG2" pin="C" pad="7"/>
<connect gate="DIG2" pin="COM@1" pad="8"/>
<connect gate="DIG2" pin="COM@2" pad="21"/>
<connect gate="DIG2" pin="D" pad="6"/>
<connect gate="DIG2" pin="DP" pad="9"/>
<connect gate="DIG2" pin="E" pad="5"/>
<connect gate="DIG2" pin="F" pad="23"/>
<connect gate="DIG2" pin="G" pad="20"/>
<connect gate="DIG3" pin="A" pad="16"/>
<connect gate="DIG3" pin="B" pad="14"/>
<connect gate="DIG3" pin="C" pad="12"/>
<connect gate="DIG3" pin="COM" pad="15"/>
<connect gate="DIG3" pin="D" pad="11"/>
<connect gate="DIG3" pin="DP" pad="13"/>
<connect gate="DIG3" pin="E" pad="10"/>
<connect gate="DIG3" pin="F" pad="17"/>
<connect gate="DIG3" pin="G" pad="18"/>
</connects>
<technologies>
<technology name="E">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="G">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="SR">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Y">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="B?56-12*WA" prefix="LED">
<description>&lt;b&gt;14.22mm (0.56INCH) THREE DIGIT NUMERIC DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com .. BA56-11EWA(Ver1189474895.pdf</description>
<gates>
<gate name="DIG1" symbol="7SEG-3-COM"/>
</gates>
<devices>
<device name="A" package="BX56-12">
<connects>
<connect gate="DIG1" pin="A" pad="11"/>
<connect gate="DIG1" pin="B" pad="7"/>
<connect gate="DIG1" pin="C" pad="4"/>
<connect gate="DIG1" pin="CA@1" pad="12"/>
<connect gate="DIG1" pin="CA@2" pad="9"/>
<connect gate="DIG1" pin="CA@3" pad="8"/>
<connect gate="DIG1" pin="D" pad="2"/>
<connect gate="DIG1" pin="DP" pad="3"/>
<connect gate="DIG1" pin="E" pad="1"/>
<connect gate="DIG1" pin="F" pad="10"/>
<connect gate="DIG1" pin="G" pad="5"/>
</connects>
<technologies>
<technology name="E">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="G">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="SR">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Y">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="C" package="BX56-12">
<connects>
<connect gate="DIG1" pin="A" pad="11"/>
<connect gate="DIG1" pin="B" pad="7"/>
<connect gate="DIG1" pin="C" pad="4"/>
<connect gate="DIG1" pin="CA@1" pad="12"/>
<connect gate="DIG1" pin="CA@2" pad="9"/>
<connect gate="DIG1" pin="CA@3" pad="8"/>
<connect gate="DIG1" pin="D" pad="2"/>
<connect gate="DIG1" pin="DP" pad="3"/>
<connect gate="DIG1" pin="E" pad="1"/>
<connect gate="DIG1" pin="F" pad="10"/>
<connect gate="DIG1" pin="G" pad="5"/>
</connects>
<technologies>
<technology name="E">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="G">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="SR">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Y">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TA20-11HWA" prefix="LED">
<description>&lt;b&gt;50mm (2.0 INCH) 5x7 DOT MATRIX DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/TC20-11EWA(Ver1189410378.9)</description>
<gates>
<gate name="G$1" symbol="DOTMATIX-35A"/>
</gates>
<devices>
<device name="" package="TA20-11HWA">
<connects>
<connect gate="G$1" pin="C1" pad="13"/>
<connect gate="G$1" pin="C2" pad="3"/>
<connect gate="G$1" pin="C3" pad="4"/>
<connect gate="G$1" pin="C3@1" pad="11"/>
<connect gate="G$1" pin="C4" pad="10"/>
<connect gate="G$1" pin="C5" pad="6"/>
<connect gate="G$1" pin="R1" pad="9"/>
<connect gate="G$1" pin="R2" pad="14"/>
<connect gate="G$1" pin="R3" pad="8"/>
<connect gate="G$1" pin="R4" pad="5"/>
<connect gate="G$1" pin="R4@1" pad="12"/>
<connect gate="G$1" pin="R5" pad="1"/>
<connect gate="G$1" pin="R6" pad="7"/>
<connect gate="G$1" pin="R7" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC20-11HWA" prefix="LED">
<description>&lt;b&gt;50mm (2.0 INCH) 5x7 DOT MATRIX DISPLAY&lt;/b&gt;&lt;p&gt;
Source: http://www.kingbright.com/manager/upload/pdf/TC20-11EWA(Ver1189410378.9)</description>
<gates>
<gate name="G$1" symbol="DOTMATIX-35C"/>
</gates>
<devices>
<device name="" package="TA20-11HWA">
<connects>
<connect gate="G$1" pin="C1" pad="13"/>
<connect gate="G$1" pin="C2" pad="3"/>
<connect gate="G$1" pin="C3" pad="4"/>
<connect gate="G$1" pin="C3@1" pad="11"/>
<connect gate="G$1" pin="C4" pad="10"/>
<connect gate="G$1" pin="C5" pad="6"/>
<connect gate="G$1" pin="R1" pad="9"/>
<connect gate="G$1" pin="R2" pad="14"/>
<connect gate="G$1" pin="R3" pad="8"/>
<connect gate="G$1" pin="R4" pad="5"/>
<connect gate="G$1" pin="R4@1" pad="12"/>
<connect gate="G$1" pin="R5" pad="1"/>
<connect gate="G$1" pin="R6" pad="7"/>
<connect gate="G$1" pin="R7" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
