<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<library>
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,3">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.3 mm with drill center</description>
</package>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
<package name="4,1">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 4.1 mm with drill center</description>
</package>
<package name="3,3-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.3 mm, round</description>
</package>
<package name="2,8-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, round</description>
</package>
<package name="4,1-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.1 mm, round</description>
</package>
<package name="3,6-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.6 mm, round</description>
</package>
<package name="3,6">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.6 mm with drill center</description>
</package>
<package name="3,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.0 mm with drill center</description>
</package>
<package name="3,0-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.0 mm, round</description>
</package>
<package name="4,5">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 4.5 mm with drill center</description>
</package>
<package name="5,0">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 5.0 mm with drill center</description>
</package>
<package name="3,2-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.2 mm, round</description>
</package>
<package name="4,3-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.3 mm, square</description>
</package>
<package name="3,3-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.3 mm, square</description>
</package>
<package name="3,0-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.0 mm, square</description>
</package>
<package name="3,2-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.2 mm, square</description>
</package>
<package name="2,8-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, square</description>
</package>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
<package name="4,3-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.3 mm, round</description>
</package>
<package name="4,5-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.5 mm, round</description>
</package>
<package name="5,5-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 5.5 mm, round</description>
</package>
<package name="3,6-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.6 mm, square</description>
</package>
<package name="4,1-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.1 mm, square</description>
</package>
<package name="5,5-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 5.5 mm, square</description>
</package>
<package name="5,0-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 5.0 mm, round</description>
</package>
<package name="5,5">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 5.5 mm with drill center</description>
</package>
<package name="5,0-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 5.0 mm, square</description>
</package>
<package name="4,3">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 4.3 mm with drill center</description>
</package>
<package name="4,5-PAD-SQUARE">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 4.5 mm, square</description>
</package>
</packages>
<symbols>
<symbol name="MOUNT-PAD">
<pin name="MOUNT" direction="pas"/>
</symbol>
<symbol name="MOUNT-HOLE">
</symbol>
<symbol name="MOUNT-PAD-SQUARE">
<pin name="MOUNT" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MOUNT-HOLE" prefix="H">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; with drill center marker</description>
<gates>
<gate name="G$1" symbol="MOUNT-HOLE"/>
</gates>
<devices>
<device name="2.8" package="2,8">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.0" package="3,0">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.3" package="3,3">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.6" package="3,6">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.1" package="4,1">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.5" package="4,5">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.0" package="5,0">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.2" package="3,2">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.3" package="4,3">
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.5" package="5,5">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOUNT-PAD-ROUND" prefix="H">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt;, round</description>
<gates>
<gate name="G$1" symbol="MOUNT-PAD"/>
</gates>
<devices>
<device name="2.8" package="2,8-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B2,8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.0" package="3,0-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,0"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.2" package="3,2-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.3" package="3,3-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.6" package="3,6-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.1" package="4,1-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.3" package="4,3-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.5" package="4,5-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.0" package="5,0-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.5" package="5,5-PAD">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B5,5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MOUNT-PAD-SQUARE" prefix="H">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt;, square</description>
<gates>
<gate name="G$1" symbol="MOUNT-PAD-SQUARE"/>
</gates>
<devices>
<device name="2.8" package="2,8-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B2,8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.0" package="3,0-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,0"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.2" package="3,2-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.3" package="3,3-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="3.6" package="3,6-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B3,6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.1" package="4,1-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.3" package="4,3-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="4.5" package="4,5-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B4,5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.0" package="5,0-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="5.5" package="5,5-PAD-SQUARE">
<connects>
<connect gate="G$1" pin="MOUNT" pad="B5,5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
