<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;PHILIPS Lumiled&lt;/b&gt; Please read the description of device and package of LUMILED_2K_TH-PAD&lt;p&gt;
Type LUXEON&lt;br&gt;
&lt;author&gt;librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LUMILED_2K">
<description>&lt;b&gt;Luxeon K2&lt;/b&gt; LED&lt;p&gt;
Source:&lt;br&gt;
0041 Luxeon K2 on FR4 with open vias.pdf&lt;br&gt;
DS60.pdf</description>
</package>
<package name="LUMILED_2K_GULLWING">
<description>&lt;b&gt;Luxeon K2 Gullwing&lt;/b&gt; LED&lt;p&gt;
Source:&lt;br&gt;
0041 Luxeon K2 on FR4 with open vias.pdf&lt;br&gt;
DS60.pdf</description>
</package>
<package name="LUMILED_2K_TH-PAD">
<description>&lt;b&gt;Luxeon K2&lt;/b&gt; LED with Thermal-Pads&lt;p&gt;
Place a Supply-Pin wit NET-Name 'TH' in schematic to connect all Thermal-Pads witout place the thermal gates.&lt;br&gt;
Place in Layout a POLYGON named 'TH' to generate a great thermal copper connected to the thermal pads.&lt;p&gt;
Source:&lt;br&gt;
0041 Luxeon K2 on FR4 with open vias.pdf&lt;br&gt;
DS60.pdf</description>
</package>
</packages>
<symbols>
<symbol name="THERMAL">
<pin name="TH" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LUMILED_2K" prefix="LED">
<description>&lt;b&gt;Luxeon K2&lt;/b&gt; LED&lt;p&gt;
Display layer 93, Pins, and connect all contact points with a net.&lt;br&gt;
The thermal pads are defined in a separate gate with addlevel REQUEST.&lt;br&gt;
Draw a net named 'TH' and connect all thermal pads with it.&lt;br&gt;
Please read the Package's Description about DRC settings.&lt;p&gt;
Source:&lt;br&gt;
0041 Luxeon K2 on FR4 with open vias.pdf&lt;br&gt;
DS60.pdf</description>
<gates>
<gate name="TH" symbol="THERMAL"/>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="" package="LUMILED_2K">
<connects>
<connect gate="G$1" pin="A" pad="1 2"/>
<connect gate="G$1" pin="C" pad="3 4"/>
<connect gate="TH" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LXK2-PB14-N00"/>
<attribute name="OC_FARNELL" value="1225059"/>
<attribute name="OC_NEWARK" value="05M0599"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUMILED_2K_GULLWING" prefix="LED">
<description>&lt;b&gt;Luxeon K2 Gullwing&lt;/b&gt; LED&lt;p&gt;
Source:&lt;br&gt;
0041 Luxeon K2 on FR4 with open vias.pdf&lt;br&gt;
DS60.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="TH" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="LUMILED_2K_GULLWING">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="C" pad="4"/>
<connect gate="TH" pin="TH" pad="TH"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LUMILED_2K_TH-30PAD" prefix="LED">
<description>&lt;b&gt;Luxeon K2&lt;/b&gt; LED with Thermal-Pads&lt;p&gt;
Place a Supply-Pin wit NET-Name 'TH' in schematic to connect all Thermal-Pads witout place the thermal gates.&lt;br&gt;
Place in Layout a POLYGON named 'TH' to generate a great thermal copper connected to the thermal pads.&lt;p&gt;
Source:&lt;br&gt;
0041 Luxeon K2 on FR4 with open vias.pdf&lt;br&gt;
DS60.pdf</description>
<gates>
<gate name="G$1" symbol="LED"/>
<gate name="G$2" symbol="THERMAL"/>
</gates>
<devices>
<device name="" package="LUMILED_2K_TH-PAD">
<connects>
<connect gate="G$1" pin="A" pad="1 2"/>
<connect gate="G$1" pin="C" pad="3 4"/>
<connect gate="G$2" pin="TH" pad="TH TH@1 TH@2 TH@3 TH@4 TH@5 TH@6 TH@7 TH@8 TH@9 TH@10 TH@11 TH@12 TH@13 TH@14 TH@15 TH@16 TH@17 TH@18 TH@19 TH@20 TH@21 TH@22 TH@23 TH@24 TH@25 TH@26 TH@27 TH@28"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LXK2-PB14-N00"/>
<attribute name="OC_FARNELL" value="1225059"/>
<attribute name="OC_NEWARK" value="05M0599"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
