<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;Static RAMs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOJ32/3">
<description>&lt;b&gt;Small Outline J-Bend&lt;/b&gt;</description>
</package>
<package name="SOJ28/3">
<description>&lt;b&gt;Small Outline J-Bend&lt;/b&gt;</description>
</package>
<package name="SOJ24/3">
<description>&lt;b&gt;Small Outline J-Bend&lt;/b&gt;</description>
</package>
<package name="SOJ32/4">
<description>&lt;b&gt;Small Outline J-Bend&lt;/b&gt;</description>
</package>
<package name="SOJ28/4">
<description>&lt;b&gt;Small Outline J-Bend&lt;/b&gt;</description>
</package>
<package name="SOP28">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL22">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="TSOPII-32">
<description>&lt;b&gt;32-pin TSOP II (51-85095)&lt;/b&gt;&lt;p&gt;
Source: Cypress CYP05780611.pdf</description>
</package>
<package name="SOJ32-400">
<description>&lt;b&gt;32-pin (400-Mil) Molded SOJ (51-85033)&lt;/b&gt;&lt;p&gt;
Source:</description>
</package>
<package name="VFBGA48">
<description>&lt;b&gt;48-ball VFBGA (6 x 8 x 1 mm) (51-85150)&lt;/b&gt;&lt;p&gt;
Source: Cypress CYP05780611.pdf</description>
</package>
<package name="DIL28-3">
<description>&lt;b&gt;Dual In Line Package Small&lt;/b&gt;</description>
</package>
<package name="DIL28-6">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt; 0.6 inch</description>
</package>
<package name="TSOP1-28">
<description>&lt;b&gt;TSOP 1-28&lt;/b&gt; 28-pin Thin Small Outline Package Type 1 (8 x 13.4 mm) (51-85071)&lt;p&gt;
Source: http://download.cypress.com.edgesuite.net/design_resources/datasheets/contents/cy62256_8.pdf</description>
</package>
<package name="TSOP1-28-R">
<description>&lt;b&gt;TSOP 1-28 R&lt;/b&gt; 28-pin Reverse Thin Small Outline Package Type 1 (8x13.4 mm) (51-85074)&lt;p&gt;
Source: http://download.cypress.com.edgesuite.net/design_resources/datasheets/contents/cy62256_8.pdf</description>
</package>
<package name="TSOPII-Z44">
<description>&lt;b&gt;44 PIN TSOP II Z44&lt;/b&gt;&lt;p&gt;
Source: CYPRESS cy7c1049cv33_8.pdf</description>
</package>
<package name="SOJV36-400">
<description>&lt;b&gt;36-Lead (400-Mil) Molded SOJ V36&lt;/b&gt;&lt;p&gt;
Source: CYPRESS cy7c1049cv33_8.pdf</description>
</package>
<package name="FBGA36">
<description>&lt;b&gt;36-Ball FBGA&lt;/b&gt; (7.00 mm x 8.5 mm x 1.2 mm) (51-85105)&lt;p&gt;
Source: CYPRESS cy7c1059dv33_8.pdf</description>
</package>
<package name="TSOPII-54">
<description>&lt;b&gt;54-pin TSOP II&lt;/b&gt; (51-85160)&lt;p&gt;
Source: CYPRESS cy7c1069av33_8.pdf</description>
</package>
<package name="FBGA60-8X20">
<description>&lt;b&gt;60-ball FBGA&lt;/b&gt; (8 mm x 20 mm x 1.2 mm) (51-85162)&lt;p&gt;
Source: CYPRESS cy7c1069av33_8.pdf</description>
</package>
</packages>
<symbols>
<symbol name="CM6705A">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="DQ8"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E1" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
</symbol>
<symbol name="PWRN">
<pin name="GND" direction="pwr"/>
<pin name="VCC" direction="pwr"/>
</symbol>
<symbol name="CM6706A">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
</symbol>
<symbol name="CM6706R">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="CM6708A">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="A15" direction="in"/>
</symbol>
<symbol name="CM6709A">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="!G" direction="in"/>
</symbol>
<symbol name="CM6709R">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A15" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="CM62V06D">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
</symbol>
<symbol name="CM6205C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="DQ8"/>
<pin name="E2" direction="in"/>
</symbol>
<symbol name="CM6207C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="D" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="Q" direction="hiz"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
</symbol>
<symbol name="CM6208C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="!W" direction="in"/>
</symbol>
<symbol name="CM6209C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A15" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
</symbol>
<symbol name="CM6226A">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="E2" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
</symbol>
<symbol name="CM6227A">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="D" direction="in"/>
<pin name="Q" direction="hiz"/>
<pin name="A19" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
</symbol>
<symbol name="CM6229A">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A15" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
</symbol>
<symbol name="CM6249">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A15" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC@2" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="CM6264C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="!E1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="E2" direction="in"/>
</symbol>
<symbol name="CM6265C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="!E1" direction="in"/>
<pin name="!G" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="DQ8"/>
<pin name="E2" direction="in"/>
</symbol>
<symbol name="CM6287B">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="D" direction="in"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="A15" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="Q" direction="hiz"/>
</symbol>
<symbol name="CM6288C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="!E" direction="in"/>
</symbol>
<symbol name="CM6290C">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="!W" direction="in"/>
<pin name="!E" direction="in"/>
<pin name="!G" direction="in"/>
</symbol>
<symbol name="LH52256">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="DQ0"/>
<pin name="DQ1"/>
<pin name="DQ2"/>
<pin name="DQ3"/>
<pin name="DQ4"/>
<pin name="DQ5"/>
<pin name="DQ6"/>
<pin name="DQ7"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="!OE" direction="in"/>
<pin name="!WE" direction="in"/>
<pin name="!CE" direction="in"/>
</symbol>
<symbol name="CY7C1019CV33">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="I/O00"/>
<pin name="I/O01"/>
<pin name="I/O02"/>
<pin name="I/O03"/>
<pin name="I/O04"/>
<pin name="I/O05"/>
<pin name="I/O06"/>
<pin name="I/O07"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="WE" direction="in" function="dot"/>
<pin name="CE" function="dot"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="+3V@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="+3V@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
</symbol>
<symbol name="4MBIT_512KX8">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="I/O00"/>
<pin name="I/O01"/>
<pin name="I/O02"/>
<pin name="I/O03"/>
<pin name="I/O04"/>
<pin name="I/O05"/>
<pin name="I/O06"/>
<pin name="I/O07"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="WE" direction="in" function="dot"/>
<pin name="CE" direction="in" function="dot"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="+3V@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="+3V@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
</symbol>
<symbol name="8MBIT_512KX8">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="I/O00"/>
<pin name="I/O01"/>
<pin name="I/O02"/>
<pin name="I/O03"/>
<pin name="I/O04"/>
<pin name="I/O05"/>
<pin name="I/O06"/>
<pin name="I/O07"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="WE" direction="in" function="dot"/>
<pin name="CE" direction="in" function="dot"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="+3V@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="+3V@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
</symbol>
<symbol name="2048KX8">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="I/O00"/>
<pin name="I/O01"/>
<pin name="I/O02"/>
<pin name="I/O03"/>
<pin name="I/O04"/>
<pin name="I/O05"/>
<pin name="I/O06"/>
<pin name="I/O07"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="WE" direction="in" function="dot"/>
<pin name="CE1" direction="in" function="dot"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="+3V@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="+3V@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="A20" direction="in"/>
<pin name="CE2" direction="in"/>
<pin name="GND@3" direction="pwr"/>
<pin name="GND@4" direction="pwr"/>
<pin name="+3V@3" direction="pwr"/>
<pin name="+3V@4" direction="pwr"/>
<pin name="+3V@5" direction="pwr"/>
<pin name="GND@5" direction="pwr"/>
<pin name="DNU" direction="pas"/>
</symbol>
<symbol name="2048KX8-FBGA60">
<pin name="A0" direction="in"/>
<pin name="A1" direction="in"/>
<pin name="A2" direction="in"/>
<pin name="A3" direction="in"/>
<pin name="A4" direction="in"/>
<pin name="A5" direction="in"/>
<pin name="A6" direction="in"/>
<pin name="A7" direction="in"/>
<pin name="A8" direction="in"/>
<pin name="I/O00"/>
<pin name="I/O01"/>
<pin name="I/O02"/>
<pin name="I/O03"/>
<pin name="I/O04"/>
<pin name="I/O05"/>
<pin name="I/O06"/>
<pin name="I/O07"/>
<pin name="A9" direction="in"/>
<pin name="A10" direction="in"/>
<pin name="A11" direction="in"/>
<pin name="A12" direction="in"/>
<pin name="A13" direction="in"/>
<pin name="A14" direction="in"/>
<pin name="WE" direction="in" function="dot"/>
<pin name="CE1" direction="in" function="dot"/>
<pin name="OE" direction="in" function="dot"/>
<pin name="A15" direction="in"/>
<pin name="A16" direction="in"/>
<pin name="+3V@1" direction="pwr"/>
<pin name="GND@1" direction="pwr"/>
<pin name="+3V@2" direction="pwr"/>
<pin name="GND@2" direction="pwr"/>
<pin name="A17" direction="in"/>
<pin name="A18" direction="in"/>
<pin name="A19" direction="in"/>
<pin name="A20" direction="in"/>
<pin name="CE2" direction="in"/>
<pin name="DNU" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MCM6705A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6705A"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ32/3">
<connects>
<connect gate="G$1" pin="!E1" pad="22"/>
<connect gate="G$1" pin="!G" pad="24"/>
<connect gate="G$1" pin="!W" pad="29"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="26"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="23"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="31"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="3"/>
<connect gate="G$1" pin="A9" pad="27"/>
<connect gate="G$1" pin="DQ0" pad="12"/>
<connect gate="G$1" pin="DQ1" pad="13"/>
<connect gate="G$1" pin="DQ2" pad="14"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="17"/>
<connect gate="G$1" pin="DQ5" pad="18"/>
<connect gate="G$1" pin="DQ6" pad="19"/>
<connect gate="G$1" pin="DQ7" pad="20"/>
<connect gate="G$1" pin="DQ8" pad="21"/>
<connect gate="G$1" pin="E2" pad="30"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6706A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6706A"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!E" pad="20"/>
<connect gate="G$1" pin="!G" pad="22"/>
<connect gate="G$1" pin="!W" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6706R" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6706R"/>
</gates>
<devices>
<device name="" package="SOJ32/3">
<connects>
<connect gate="G$1" pin="!E" pad="5"/>
<connect gate="G$1" pin="!G" pad="28"/>
<connect gate="G$1" pin="!W" pad="12"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="20"/>
<connect gate="G$1" pin="A11" pad="21"/>
<connect gate="G$1" pin="A12" pad="29"/>
<connect gate="G$1" pin="A13" pad="30"/>
<connect gate="G$1" pin="A14" pad="31"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="14"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="16"/>
<connect gate="G$1" pin="A8" pad="18"/>
<connect gate="G$1" pin="A9" pad="19"/>
<connect gate="G$1" pin="DQ0" pad="6"/>
<connect gate="G$1" pin="DQ1" pad="7"/>
<connect gate="G$1" pin="DQ2" pad="10"/>
<connect gate="G$1" pin="DQ3" pad="11"/>
<connect gate="G$1" pin="DQ4" pad="22"/>
<connect gate="G$1" pin="DQ5" pad="23"/>
<connect gate="G$1" pin="DQ6" pad="26"/>
<connect gate="G$1" pin="DQ7" pad="27"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="VCC@1" pad="8"/>
<connect gate="G$1" pin="VCC@2" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6708A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G$1" symbol="CM6708A"/>
</gates>
<devices>
<device name="" package="SOJ24/3">
<connects>
<connect gate="G$1" pin="!E" pad="11"/>
<connect gate="G$1" pin="!W" pad="13"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="18"/>
<connect gate="G$1" pin="A11" pad="19"/>
<connect gate="G$1" pin="A12" pad="20"/>
<connect gate="G$1" pin="A13" pad="21"/>
<connect gate="G$1" pin="A14" pad="22"/>
<connect gate="G$1" pin="A15" pad="23"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="10"/>
<connect gate="G$1" pin="DQ0" pad="17"/>
<connect gate="G$1" pin="DQ1" pad="16"/>
<connect gate="G$1" pin="DQ2" pad="15"/>
<connect gate="G$1" pin="DQ3" pad="14"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6709A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6709A"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!E" pad="12"/>
<connect gate="G$1" pin="!G" pad="13"/>
<connect gate="G$1" pin="!W" pad="15"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A10" pad="22"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="24"/>
<connect gate="G$1" pin="A13" pad="25"/>
<connect gate="G$1" pin="A14" pad="26"/>
<connect gate="G$1" pin="A15" pad="27"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="10"/>
<connect gate="G$1" pin="A9" pad="11"/>
<connect gate="G$1" pin="DQ0" pad="19"/>
<connect gate="G$1" pin="DQ1" pad="18"/>
<connect gate="G$1" pin="DQ2" pad="17"/>
<connect gate="G$1" pin="DQ3" pad="16"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6709R" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6709R"/>
</gates>
<devices>
<device name="" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!E" pad="5"/>
<connect gate="G$1" pin="!G" pad="24"/>
<connect gate="G$1" pin="!W" pad="10"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="18"/>
<connect gate="G$1" pin="A11" pad="19"/>
<connect gate="G$1" pin="A12" pad="25"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="28"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="11"/>
<connect gate="G$1" pin="A5" pad="12"/>
<connect gate="G$1" pin="A6" pad="13"/>
<connect gate="G$1" pin="A7" pad="14"/>
<connect gate="G$1" pin="A8" pad="16"/>
<connect gate="G$1" pin="A9" pad="17"/>
<connect gate="G$1" pin="DQ0" pad="6"/>
<connect gate="G$1" pin="DQ1" pad="9"/>
<connect gate="G$1" pin="DQ2" pad="20"/>
<connect gate="G$1" pin="DQ3" pad="23"/>
<connect gate="G$1" pin="GND@1" pad="8"/>
<connect gate="G$1" pin="GND@2" pad="22"/>
<connect gate="G$1" pin="VCC@1" pad="7"/>
<connect gate="G$1" pin="VCC@2" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM62V06D" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM62V06D"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!E" pad="20"/>
<connect gate="G$1" pin="!G" pad="22"/>
<connect gate="G$1" pin="!W" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6205C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6205C"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ32/3">
<connects>
<connect gate="G$1" pin="!E1" pad="22"/>
<connect gate="G$1" pin="!G" pad="24"/>
<connect gate="G$1" pin="!W" pad="29"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="26"/>
<connect gate="G$1" pin="A11" pad="25"/>
<connect gate="G$1" pin="A12" pad="23"/>
<connect gate="G$1" pin="A13" pad="28"/>
<connect gate="G$1" pin="A14" pad="31"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="4"/>
<connect gate="G$1" pin="A8" pad="3"/>
<connect gate="G$1" pin="A9" pad="27"/>
<connect gate="G$1" pin="DQ0" pad="12"/>
<connect gate="G$1" pin="DQ1" pad="13"/>
<connect gate="G$1" pin="DQ2" pad="14"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="17"/>
<connect gate="G$1" pin="DQ5" pad="18"/>
<connect gate="G$1" pin="DQ6" pad="19"/>
<connect gate="G$1" pin="DQ7" pad="20"/>
<connect gate="G$1" pin="DQ8" pad="21"/>
<connect gate="G$1" pin="E2" pad="30"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6206C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM62V06D"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!E" pad="20"/>
<connect gate="G$1" pin="!G" pad="22"/>
<connect gate="G$1" pin="!W" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6207C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6207C"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ24/3">
<connects>
<connect gate="G$1" pin="!E" pad="13"/>
<connect gate="G$1" pin="!W" pad="11"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="16"/>
<connect gate="G$1" pin="A11" pad="17"/>
<connect gate="G$1" pin="A12" pad="18"/>
<connect gate="G$1" pin="A13" pad="19"/>
<connect gate="G$1" pin="A14" pad="20"/>
<connect gate="G$1" pin="A15" pad="21"/>
<connect gate="G$1" pin="A16" pad="22"/>
<connect gate="G$1" pin="A17" pad="23"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="15"/>
<connect gate="G$1" pin="D" pad="14"/>
<connect gate="G$1" pin="Q" pad="10"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6208C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6208C"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ24/3">
<connects>
<connect gate="G$1" pin="!E" pad="11"/>
<connect gate="G$1" pin="!W" pad="13"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="18"/>
<connect gate="G$1" pin="A11" pad="19"/>
<connect gate="G$1" pin="A12" pad="20"/>
<connect gate="G$1" pin="A13" pad="21"/>
<connect gate="G$1" pin="A14" pad="22"/>
<connect gate="G$1" pin="A15" pad="23"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="10"/>
<connect gate="G$1" pin="DQ0" pad="17"/>
<connect gate="G$1" pin="DQ1" pad="16"/>
<connect gate="G$1" pin="DQ2" pad="15"/>
<connect gate="G$1" pin="DQ3" pad="14"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6209C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6209C"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!E" pad="12"/>
<connect gate="G$1" pin="!G" pad="13"/>
<connect gate="G$1" pin="!W" pad="15"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A10" pad="22"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="24"/>
<connect gate="G$1" pin="A13" pad="25"/>
<connect gate="G$1" pin="A14" pad="26"/>
<connect gate="G$1" pin="A15" pad="27"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="10"/>
<connect gate="G$1" pin="A9" pad="11"/>
<connect gate="G$1" pin="DQ0" pad="19"/>
<connect gate="G$1" pin="DQ1" pad="18"/>
<connect gate="G$1" pin="DQ2" pad="17"/>
<connect gate="G$1" pin="DQ3" pad="16"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6226A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6226A"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ32/4">
<connects>
<connect gate="G$1" pin="!E1" pad="22"/>
<connect gate="G$1" pin="!G" pad="24"/>
<connect gate="G$1" pin="!W" pad="29"/>
<connect gate="G$1" pin="A0" pad="2"/>
<connect gate="G$1" pin="A1" pad="3"/>
<connect gate="G$1" pin="A10" pad="12"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="25"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="27"/>
<connect gate="G$1" pin="A15" pad="28"/>
<connect gate="G$1" pin="A16" pad="31"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="A3" pad="5"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="7"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="10"/>
<connect gate="G$1" pin="A9" pad="11"/>
<connect gate="G$1" pin="DQ0" pad="13"/>
<connect gate="G$1" pin="DQ1" pad="14"/>
<connect gate="G$1" pin="DQ2" pad="15"/>
<connect gate="G$1" pin="DQ3" pad="17"/>
<connect gate="G$1" pin="DQ4" pad="18"/>
<connect gate="G$1" pin="DQ5" pad="19"/>
<connect gate="G$1" pin="DQ6" pad="20"/>
<connect gate="G$1" pin="DQ7" pad="21"/>
<connect gate="G$1" pin="E2" pad="30"/>
<connect gate="P" pin="GND" pad="16"/>
<connect gate="P" pin="VCC" pad="32"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6227A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6227A"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/4">
<connects>
<connect gate="G$1" pin="!E" pad="15"/>
<connect gate="G$1" pin="!W" pad="13"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="17"/>
<connect gate="G$1" pin="A11" pad="18"/>
<connect gate="G$1" pin="A12" pad="19"/>
<connect gate="G$1" pin="A13" pad="20"/>
<connect gate="G$1" pin="A14" pad="22"/>
<connect gate="G$1" pin="A15" pad="23"/>
<connect gate="G$1" pin="A16" pad="24"/>
<connect gate="G$1" pin="A17" pad="25"/>
<connect gate="G$1" pin="A18" pad="26"/>
<connect gate="G$1" pin="A19" pad="27"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="10"/>
<connect gate="G$1" pin="A9" pad="11"/>
<connect gate="G$1" pin="D" pad="16"/>
<connect gate="G$1" pin="Q" pad="12"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6229A" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6229A"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/4">
<connects>
<connect gate="G$1" pin="!E" pad="12"/>
<connect gate="G$1" pin="!G" pad="13"/>
<connect gate="G$1" pin="!W" pad="15"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="11"/>
<connect gate="G$1" pin="A11" pad="21"/>
<connect gate="G$1" pin="A12" pad="22"/>
<connect gate="G$1" pin="A13" pad="23"/>
<connect gate="G$1" pin="A14" pad="24"/>
<connect gate="G$1" pin="A15" pad="25"/>
<connect gate="G$1" pin="A16" pad="26"/>
<connect gate="G$1" pin="A17" pad="27"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="10"/>
<connect gate="G$1" pin="DQ0" pad="16"/>
<connect gate="G$1" pin="DQ1" pad="17"/>
<connect gate="G$1" pin="DQ2" pad="18"/>
<connect gate="G$1" pin="DQ3" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6249" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6249"/>
</gates>
<devices>
<device name="" package="SOJ32/4">
<connects>
<connect gate="G$1" pin="!E" pad="6"/>
<connect gate="G$1" pin="!G" pad="27"/>
<connect gate="G$1" pin="!W" pad="11"/>
<connect gate="G$1" pin="A0" pad="31"/>
<connect gate="G$1" pin="A1" pad="32"/>
<connect gate="G$1" pin="A10" pad="14"/>
<connect gate="G$1" pin="A11" pad="15"/>
<connect gate="G$1" pin="A12" pad="16"/>
<connect gate="G$1" pin="A13" pad="12"/>
<connect gate="G$1" pin="A14" pad="19"/>
<connect gate="G$1" pin="A15" pad="20"/>
<connect gate="G$1" pin="A16" pad="21"/>
<connect gate="G$1" pin="A17" pad="4"/>
<connect gate="G$1" pin="A18" pad="13"/>
<connect gate="G$1" pin="A19" pad="28"/>
<connect gate="G$1" pin="A2" pad="22"/>
<connect gate="G$1" pin="A3" pad="18"/>
<connect gate="G$1" pin="A4" pad="29"/>
<connect gate="G$1" pin="A5" pad="30"/>
<connect gate="G$1" pin="A6" pad="5"/>
<connect gate="G$1" pin="A7" pad="1"/>
<connect gate="G$1" pin="A8" pad="2"/>
<connect gate="G$1" pin="A9" pad="3"/>
<connect gate="G$1" pin="DQ0" pad="7"/>
<connect gate="G$1" pin="DQ1" pad="10"/>
<connect gate="G$1" pin="DQ2" pad="23"/>
<connect gate="G$1" pin="DQ3" pad="26"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="VCC@1" pad="8"/>
<connect gate="G$1" pin="VCC@2" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6264C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6264C"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!E1" pad="20"/>
<connect gate="G$1" pin="!G" pad="22"/>
<connect gate="G$1" pin="!W" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="G$1" pin="E2" pad="26"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6265C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6265C"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!E1" pad="20"/>
<connect gate="G$1" pin="!G" pad="22"/>
<connect gate="G$1" pin="!W" pad="27"/>
<connect gate="G$1" pin="A0" pad="9"/>
<connect gate="G$1" pin="A1" pad="8"/>
<connect gate="G$1" pin="A10" pad="24"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="21"/>
<connect gate="G$1" pin="A2" pad="7"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="4"/>
<connect gate="G$1" pin="A6" pad="3"/>
<connect gate="G$1" pin="A7" pad="2"/>
<connect gate="G$1" pin="A8" pad="1"/>
<connect gate="G$1" pin="A9" pad="25"/>
<connect gate="G$1" pin="DQ0" pad="10"/>
<connect gate="G$1" pin="DQ1" pad="11"/>
<connect gate="G$1" pin="DQ2" pad="12"/>
<connect gate="G$1" pin="DQ3" pad="13"/>
<connect gate="G$1" pin="DQ4" pad="15"/>
<connect gate="G$1" pin="DQ5" pad="16"/>
<connect gate="G$1" pin="DQ6" pad="17"/>
<connect gate="G$1" pin="DQ7" pad="18"/>
<connect gate="G$1" pin="DQ8" pad="19"/>
<connect gate="G$1" pin="E2" pad="26"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6287B" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6287B"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ24/3">
<connects>
<connect gate="G$1" pin="!E" pad="13"/>
<connect gate="G$1" pin="!W" pad="11"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="17"/>
<connect gate="G$1" pin="A11" pad="18"/>
<connect gate="G$1" pin="A12" pad="20"/>
<connect gate="G$1" pin="A13" pad="21"/>
<connect gate="G$1" pin="A14" pad="22"/>
<connect gate="G$1" pin="A15" pad="23"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="8"/>
<connect gate="G$1" pin="A7" pad="9"/>
<connect gate="G$1" pin="A8" pad="15"/>
<connect gate="G$1" pin="A9" pad="16"/>
<connect gate="G$1" pin="D" pad="14"/>
<connect gate="G$1" pin="Q" pad="10"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6288C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6288C"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="DIL22">
<connects>
<connect gate="G$1" pin="!E" pad="10"/>
<connect gate="G$1" pin="!W" pad="12"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="18"/>
<connect gate="G$1" pin="A11" pad="19"/>
<connect gate="G$1" pin="A12" pad="20"/>
<connect gate="G$1" pin="A13" pad="21"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="17"/>
<connect gate="G$1" pin="DQ0" pad="16"/>
<connect gate="G$1" pin="DQ1" pad="15"/>
<connect gate="G$1" pin="DQ2" pad="14"/>
<connect gate="G$1" pin="DQ3" pad="13"/>
<connect gate="P" pin="GND" pad="11"/>
<connect gate="P" pin="VCC" pad="22"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCM6290C" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="CM6290C"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="" package="SOJ24/3">
<connects>
<connect gate="G$1" pin="!E" pad="10"/>
<connect gate="G$1" pin="!G" pad="11"/>
<connect gate="G$1" pin="!W" pad="13"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="20"/>
<connect gate="G$1" pin="A11" pad="21"/>
<connect gate="G$1" pin="A12" pad="22"/>
<connect gate="G$1" pin="A13" pad="23"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="6"/>
<connect gate="G$1" pin="A6" pad="7"/>
<connect gate="G$1" pin="A7" pad="8"/>
<connect gate="G$1" pin="A8" pad="9"/>
<connect gate="G$1" pin="A9" pad="19"/>
<connect gate="G$1" pin="DQ0" pad="17"/>
<connect gate="G$1" pin="DQ1" pad="16"/>
<connect gate="G$1" pin="DQ2" pad="15"/>
<connect gate="G$1" pin="DQ3" pad="14"/>
<connect gate="P" pin="GND" pad="12"/>
<connect gate="P" pin="VCC" pad="24"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LH52256CHN" prefix="IC" uservalue="yes">
<description>&lt;b&gt;MEMORY&lt;/b&gt;</description>
<gates>
<gate name="P" symbol="PWRN"/>
<gate name="G$1" symbol="LH52256"/>
</gates>
<devices>
<device name="" package="SOP28">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="10"/>
<connect gate="G$1" pin="A1" pad="9"/>
<connect gate="G$1" pin="A10" pad="21"/>
<connect gate="G$1" pin="A11" pad="23"/>
<connect gate="G$1" pin="A12" pad="2"/>
<connect gate="G$1" pin="A13" pad="26"/>
<connect gate="G$1" pin="A14" pad="1"/>
<connect gate="G$1" pin="A2" pad="8"/>
<connect gate="G$1" pin="A3" pad="7"/>
<connect gate="G$1" pin="A4" pad="6"/>
<connect gate="G$1" pin="A5" pad="5"/>
<connect gate="G$1" pin="A6" pad="4"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="25"/>
<connect gate="G$1" pin="A9" pad="24"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C1019CV33" prefix="IC">
<description>&lt;b&gt;128K x 8 Static RAM&lt;/b&gt; 10ns&lt;p&gt;
Source: Cypress CYP05780611.pdf</description>
<gates>
<gate name="G$1" symbol="CY7C1019CV33"/>
</gates>
<devices>
<device name="ZXC" package="TSOPII-32">
<connects>
<connect gate="G$1" pin="+3V@1" pad="8"/>
<connect gate="G$1" pin="+3V@2" pad="24"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="19"/>
<connect gate="G$1" pin="A11" pad="20"/>
<connect gate="G$1" pin="A12" pad="21"/>
<connect gate="G$1" pin="A13" pad="29"/>
<connect gate="G$1" pin="A14" pad="30"/>
<connect gate="G$1" pin="A15" pad="31"/>
<connect gate="G$1" pin="A16" pad="32"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="14"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="16"/>
<connect gate="G$1" pin="A8" pad="17"/>
<connect gate="G$1" pin="A9" pad="18"/>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="I/O00" pad="6"/>
<connect gate="G$1" pin="I/O01" pad="7"/>
<connect gate="G$1" pin="I/O02" pad="10"/>
<connect gate="G$1" pin="I/O03" pad="11"/>
<connect gate="G$1" pin="I/O04" pad="22"/>
<connect gate="G$1" pin="I/O05" pad="23"/>
<connect gate="G$1" pin="I/O06" pad="26"/>
<connect gate="G$1" pin="I/O07" pad="27"/>
<connect gate="G$1" pin="OE" pad="28"/>
<connect gate="G$1" pin="WE" pad="12"/>
</connects>
<technologies>
<technology name=""/>
<technology name="-10"/>
<technology name="-12"/>
<technology name="-15"/>
</technologies>
</device>
<device name="VC" package="SOJ32-400">
<connects>
<connect gate="G$1" pin="+3V@1" pad="8"/>
<connect gate="G$1" pin="+3V@2" pad="24"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="19"/>
<connect gate="G$1" pin="A11" pad="20"/>
<connect gate="G$1" pin="A12" pad="21"/>
<connect gate="G$1" pin="A13" pad="29"/>
<connect gate="G$1" pin="A14" pad="30"/>
<connect gate="G$1" pin="A15" pad="31"/>
<connect gate="G$1" pin="A16" pad="32"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="13"/>
<connect gate="G$1" pin="A5" pad="14"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="16"/>
<connect gate="G$1" pin="A8" pad="17"/>
<connect gate="G$1" pin="A9" pad="18"/>
<connect gate="G$1" pin="CE" pad="5"/>
<connect gate="G$1" pin="GND@1" pad="9"/>
<connect gate="G$1" pin="GND@2" pad="25"/>
<connect gate="G$1" pin="I/O00" pad="6"/>
<connect gate="G$1" pin="I/O01" pad="7"/>
<connect gate="G$1" pin="I/O02" pad="10"/>
<connect gate="G$1" pin="I/O03" pad="11"/>
<connect gate="G$1" pin="I/O04" pad="22"/>
<connect gate="G$1" pin="I/O05" pad="23"/>
<connect gate="G$1" pin="I/O06" pad="26"/>
<connect gate="G$1" pin="I/O07" pad="27"/>
<connect gate="G$1" pin="OE" pad="28"/>
<connect gate="G$1" pin="WE" pad="12"/>
</connects>
<technologies>
<technology name="-10"/>
<technology name="-12"/>
<technology name="-15"/>
</technologies>
</device>
<device name="BVXI" package="VFBGA48">
<connects>
<connect gate="G$1" pin="+3V@1" pad="D6"/>
<connect gate="G$1" pin="+3V@2" pad="E1"/>
<connect gate="G$1" pin="A0" pad="C3"/>
<connect gate="G$1" pin="A1" pad="B3"/>
<connect gate="G$1" pin="A10" pad="H2"/>
<connect gate="G$1" pin="A11" pad="F4"/>
<connect gate="G$1" pin="A12" pad="G4"/>
<connect gate="G$1" pin="A13" pad="H4"/>
<connect gate="G$1" pin="A14" pad="F3"/>
<connect gate="G$1" pin="A15" pad="G3"/>
<connect gate="G$1" pin="A16" pad="H3"/>
<connect gate="G$1" pin="A2" pad="A3"/>
<connect gate="G$1" pin="A3" pad="D4"/>
<connect gate="G$1" pin="A4" pad="C4"/>
<connect gate="G$1" pin="A5" pad="B4"/>
<connect gate="G$1" pin="A6" pad="A4"/>
<connect gate="G$1" pin="A7" pad="A5"/>
<connect gate="G$1" pin="A8" pad="G6"/>
<connect gate="G$1" pin="A9" pad="H5"/>
<connect gate="G$1" pin="CE" pad="B5"/>
<connect gate="G$1" pin="GND@1" pad="D1"/>
<connect gate="G$1" pin="GND@2" pad="E6"/>
<connect gate="G$1" pin="I/O00" pad="B1"/>
<connect gate="G$1" pin="I/O01" pad="C1"/>
<connect gate="G$1" pin="I/O02" pad="F1"/>
<connect gate="G$1" pin="I/O03" pad="G1"/>
<connect gate="G$1" pin="I/O04" pad="F5"/>
<connect gate="G$1" pin="I/O05" pad="F6"/>
<connect gate="G$1" pin="I/O06" pad="C6"/>
<connect gate="G$1" pin="I/O07" pad="B6"/>
<connect gate="G$1" pin="OE" pad="A2"/>
<connect gate="G$1" pin="WE" pad="G5"/>
</connects>
<technologies>
<technology name="-12"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY62256LL-?*" prefix="IC">
<description>&lt;b&gt;256K (32K x 8) CMOS-Static RAM&lt;/b&gt;&lt;p&gt;
Source: http://download.cypress.com.edgesuite.net/design_resources/datasheets/contents/cy62256_8.pdf</description>
<gates>
<gate name="G$1" symbol="LH52256"/>
<gate name="P" symbol="PWRN"/>
</gates>
<devices>
<device name="S" package="SOJ28/3">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A10" pad="6"/>
<connect gate="G$1" pin="A11" pad="7"/>
<connect gate="G$1" pin="A12" pad="8"/>
<connect gate="G$1" pin="A13" pad="9"/>
<connect gate="G$1" pin="A14" pad="10"/>
<connect gate="G$1" pin="A2" pad="24"/>
<connect gate="G$1" pin="A3" pad="25"/>
<connect gate="G$1" pin="A4" pad="26"/>
<connect gate="G$1" pin="A5" pad="1"/>
<connect gate="G$1" pin="A6" pad="2"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="5"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="NC"/>
<technology name="NE"/>
<technology name="NI"/>
<technology name="NXC"/>
<technology name="NXE"/>
<technology name="NXI"/>
</technologies>
</device>
<device name="P" package="DIL28-6">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A10" pad="6"/>
<connect gate="G$1" pin="A11" pad="7"/>
<connect gate="G$1" pin="A12" pad="8"/>
<connect gate="G$1" pin="A13" pad="9"/>
<connect gate="G$1" pin="A14" pad="10"/>
<connect gate="G$1" pin="A2" pad="24"/>
<connect gate="G$1" pin="A3" pad="25"/>
<connect gate="G$1" pin="A4" pad="26"/>
<connect gate="G$1" pin="A5" pad="1"/>
<connect gate="G$1" pin="A6" pad="2"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="5"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="XC"/>
</technologies>
</device>
<device name="Z" package="TSOP1-28">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A10" pad="6"/>
<connect gate="G$1" pin="A11" pad="7"/>
<connect gate="G$1" pin="A12" pad="8"/>
<connect gate="G$1" pin="A13" pad="9"/>
<connect gate="G$1" pin="A14" pad="10"/>
<connect gate="G$1" pin="A2" pad="24"/>
<connect gate="G$1" pin="A3" pad="25"/>
<connect gate="G$1" pin="A4" pad="26"/>
<connect gate="G$1" pin="A5" pad="1"/>
<connect gate="G$1" pin="A6" pad="2"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="5"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="C"/>
<technology name="E"/>
<technology name="XC"/>
<technology name="XE"/>
<technology name="XI"/>
</technologies>
</device>
<device name="ZR" package="TSOP1-28-R">
<connects>
<connect gate="G$1" pin="!CE" pad="20"/>
<connect gate="G$1" pin="!OE" pad="22"/>
<connect gate="G$1" pin="!WE" pad="27"/>
<connect gate="G$1" pin="A0" pad="21"/>
<connect gate="G$1" pin="A1" pad="23"/>
<connect gate="G$1" pin="A10" pad="6"/>
<connect gate="G$1" pin="A11" pad="7"/>
<connect gate="G$1" pin="A12" pad="8"/>
<connect gate="G$1" pin="A13" pad="9"/>
<connect gate="G$1" pin="A14" pad="10"/>
<connect gate="G$1" pin="A2" pad="24"/>
<connect gate="G$1" pin="A3" pad="25"/>
<connect gate="G$1" pin="A4" pad="26"/>
<connect gate="G$1" pin="A5" pad="1"/>
<connect gate="G$1" pin="A6" pad="2"/>
<connect gate="G$1" pin="A7" pad="3"/>
<connect gate="G$1" pin="A8" pad="4"/>
<connect gate="G$1" pin="A9" pad="5"/>
<connect gate="G$1" pin="DQ0" pad="11"/>
<connect gate="G$1" pin="DQ1" pad="12"/>
<connect gate="G$1" pin="DQ2" pad="13"/>
<connect gate="G$1" pin="DQ3" pad="15"/>
<connect gate="G$1" pin="DQ4" pad="16"/>
<connect gate="G$1" pin="DQ5" pad="17"/>
<connect gate="G$1" pin="DQ6" pad="18"/>
<connect gate="G$1" pin="DQ7" pad="19"/>
<connect gate="P" pin="GND" pad="14"/>
<connect gate="P" pin="VCC" pad="28"/>
</connects>
<technologies>
<technology name="I"/>
<technology name="XE"/>
<technology name="XI"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C1049CV33" prefix="IC">
<description>&lt;b&gt;4-Mbit (512K x 8) Static RAM&lt;/b&gt;&lt;p&gt;
Source: CYPRESS cy7c1049cv33_8.pdf</description>
<gates>
<gate name="G$1" symbol="4MBIT_512KX8"/>
</gates>
<devices>
<device name="" package="SOJV36-400">
<connects>
<connect gate="G$1" pin="+3V@1" pad="9"/>
<connect gate="G$1" pin="+3V@2" pad="27"/>
<connect gate="G$1" pin="A0" pad="1"/>
<connect gate="G$1" pin="A1" pad="2"/>
<connect gate="G$1" pin="A10" pad="20"/>
<connect gate="G$1" pin="A11" pad="21"/>
<connect gate="G$1" pin="A12" pad="22"/>
<connect gate="G$1" pin="A13" pad="23"/>
<connect gate="G$1" pin="A14" pad="24"/>
<connect gate="G$1" pin="A15" pad="32"/>
<connect gate="G$1" pin="A16" pad="33"/>
<connect gate="G$1" pin="A17" pad="34"/>
<connect gate="G$1" pin="A18" pad="35"/>
<connect gate="G$1" pin="A2" pad="3"/>
<connect gate="G$1" pin="A3" pad="4"/>
<connect gate="G$1" pin="A4" pad="5"/>
<connect gate="G$1" pin="A5" pad="14"/>
<connect gate="G$1" pin="A6" pad="15"/>
<connect gate="G$1" pin="A7" pad="16"/>
<connect gate="G$1" pin="A8" pad="17"/>
<connect gate="G$1" pin="A9" pad="18"/>
<connect gate="G$1" pin="CE" pad="6"/>
<connect gate="G$1" pin="GND@1" pad="10"/>
<connect gate="G$1" pin="GND@2" pad="28"/>
<connect gate="G$1" pin="I/O00" pad="7"/>
<connect gate="G$1" pin="I/O01" pad="8"/>
<connect gate="G$1" pin="I/O02" pad="11"/>
<connect gate="G$1" pin="I/O03" pad="12"/>
<connect gate="G$1" pin="I/O04" pad="25"/>
<connect gate="G$1" pin="I/O05" pad="26"/>
<connect gate="G$1" pin="I/O06" pad="29"/>
<connect gate="G$1" pin="I/O07" pad="30"/>
<connect gate="G$1" pin="OE" pad="31"/>
<connect gate="G$1" pin="WE" pad="13"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="TSOPII-Z44">
<connects>
<connect gate="G$1" pin="+3V@1" pad="11"/>
<connect gate="G$1" pin="+3V@2" pad="33"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A10" pad="26"/>
<connect gate="G$1" pin="A11" pad="27"/>
<connect gate="G$1" pin="A12" pad="28"/>
<connect gate="G$1" pin="A13" pad="29"/>
<connect gate="G$1" pin="A14" pad="30"/>
<connect gate="G$1" pin="A15" pad="38"/>
<connect gate="G$1" pin="A16" pad="39"/>
<connect gate="G$1" pin="A17" pad="40"/>
<connect gate="G$1" pin="A18" pad="41"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="16"/>
<connect gate="G$1" pin="A6" pad="17"/>
<connect gate="G$1" pin="A7" pad="18"/>
<connect gate="G$1" pin="A8" pad="19"/>
<connect gate="G$1" pin="A9" pad="20"/>
<connect gate="G$1" pin="CE" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="34"/>
<connect gate="G$1" pin="I/O00" pad="9"/>
<connect gate="G$1" pin="I/O01" pad="10"/>
<connect gate="G$1" pin="I/O02" pad="13"/>
<connect gate="G$1" pin="I/O03" pad="14"/>
<connect gate="G$1" pin="I/O04" pad="31"/>
<connect gate="G$1" pin="I/O05" pad="32"/>
<connect gate="G$1" pin="I/O06" pad="35"/>
<connect gate="G$1" pin="I/O07" pad="36"/>
<connect gate="G$1" pin="OE" pad="37"/>
<connect gate="G$1" pin="WE" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C1059DV33" prefix="IC">
<description>Source: CYPRESS cy7c1059dv33_8.pdf</description>
<gates>
<gate name="G$1" symbol="8MBIT_512KX8"/>
</gates>
<devices>
<device name="-10ZSXI" package="TSOPII-Z44">
<connects>
<connect gate="G$1" pin="+3V@1" pad="11"/>
<connect gate="G$1" pin="+3V@2" pad="33"/>
<connect gate="G$1" pin="A0" pad="3"/>
<connect gate="G$1" pin="A1" pad="4"/>
<connect gate="G$1" pin="A10" pad="26"/>
<connect gate="G$1" pin="A11" pad="27"/>
<connect gate="G$1" pin="A12" pad="28"/>
<connect gate="G$1" pin="A13" pad="29"/>
<connect gate="G$1" pin="A14" pad="30"/>
<connect gate="G$1" pin="A15" pad="38"/>
<connect gate="G$1" pin="A16" pad="39"/>
<connect gate="G$1" pin="A17" pad="40"/>
<connect gate="G$1" pin="A18" pad="41"/>
<connect gate="G$1" pin="A19" pad="25"/>
<connect gate="G$1" pin="A2" pad="5"/>
<connect gate="G$1" pin="A3" pad="6"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="16"/>
<connect gate="G$1" pin="A6" pad="17"/>
<connect gate="G$1" pin="A7" pad="18"/>
<connect gate="G$1" pin="A8" pad="19"/>
<connect gate="G$1" pin="A9" pad="20"/>
<connect gate="G$1" pin="CE" pad="8"/>
<connect gate="G$1" pin="GND@1" pad="12"/>
<connect gate="G$1" pin="GND@2" pad="34"/>
<connect gate="G$1" pin="I/O00" pad="9"/>
<connect gate="G$1" pin="I/O01" pad="10"/>
<connect gate="G$1" pin="I/O02" pad="13"/>
<connect gate="G$1" pin="I/O03" pad="14"/>
<connect gate="G$1" pin="I/O04" pad="31"/>
<connect gate="G$1" pin="I/O05" pad="32"/>
<connect gate="G$1" pin="I/O06" pad="35"/>
<connect gate="G$1" pin="I/O07" pad="36"/>
<connect gate="G$1" pin="OE" pad="37"/>
<connect gate="G$1" pin="WE" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-10BAXI" package="FBGA36">
<connects>
<connect gate="G$1" pin="+3V@1" pad="D6"/>
<connect gate="G$1" pin="+3V@2" pad="E1"/>
<connect gate="G$1" pin="A0" pad="A1"/>
<connect gate="G$1" pin="A1" pad="A2"/>
<connect gate="G$1" pin="A10" pad="H2"/>
<connect gate="G$1" pin="A11" pad="H3"/>
<connect gate="G$1" pin="A12" pad="H4"/>
<connect gate="G$1" pin="A13" pad="H5"/>
<connect gate="G$1" pin="A14" pad="H6"/>
<connect gate="G$1" pin="A15" pad="G5"/>
<connect gate="G$1" pin="A16" pad="G4"/>
<connect gate="G$1" pin="A17" pad="F4"/>
<connect gate="G$1" pin="A18" pad="F3"/>
<connect gate="G$1" pin="A19" pad="C3"/>
<connect gate="G$1" pin="A2" pad="B2"/>
<connect gate="G$1" pin="A3" pad="A4"/>
<connect gate="G$1" pin="A4" pad="B4"/>
<connect gate="G$1" pin="A5" pad="C4"/>
<connect gate="G$1" pin="A6" pad="A5"/>
<connect gate="G$1" pin="A7" pad="B5"/>
<connect gate="G$1" pin="A8" pad="A6"/>
<connect gate="G$1" pin="A9" pad="H1"/>
<connect gate="G$1" pin="CE" pad="G3"/>
<connect gate="G$1" pin="GND@1" pad="D1"/>
<connect gate="G$1" pin="GND@2" pad="E6"/>
<connect gate="G$1" pin="I/O00" pad="B6"/>
<connect gate="G$1" pin="I/O01" pad="C6"/>
<connect gate="G$1" pin="I/O02" pad="F6"/>
<connect gate="G$1" pin="I/O03" pad="G6"/>
<connect gate="G$1" pin="I/O04" pad="B1"/>
<connect gate="G$1" pin="I/O05" pad="C1"/>
<connect gate="G$1" pin="I/O06" pad="F1"/>
<connect gate="G$1" pin="I/O07" pad="G1"/>
<connect gate="G$1" pin="OE" pad="G2"/>
<connect gate="G$1" pin="WE" pad="B3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C1069AV33Z" prefix="IC">
<description>&lt;b&gt;2M x 8 Static RAM&lt;/b&gt;&lt;p&gt;
Source: CYPRESS cy7c1069av33_8.pdf</description>
<gates>
<gate name="G$1" symbol="2048KX8"/>
</gates>
<devices>
<device name="" package="TSOPII-54">
<connects>
<connect gate="G$1" pin="+3V@1" pad="2"/>
<connect gate="G$1" pin="+3V@2" pad="14"/>
<connect gate="G$1" pin="+3V@3" pad="23"/>
<connect gate="G$1" pin="+3V@4" pad="29"/>
<connect gate="G$1" pin="+3V@5" pad="50"/>
<connect gate="G$1" pin="A0" pad="11"/>
<connect gate="G$1" pin="A1" pad="10"/>
<connect gate="G$1" pin="A10" pad="38"/>
<connect gate="G$1" pin="A11" pad="37"/>
<connect gate="G$1" pin="A12" pad="36"/>
<connect gate="G$1" pin="A13" pad="35"/>
<connect gate="G$1" pin="A14" pad="34"/>
<connect gate="G$1" pin="A15" pad="21"/>
<connect gate="G$1" pin="A16" pad="20"/>
<connect gate="G$1" pin="A17" pad="19"/>
<connect gate="G$1" pin="A18" pad="18"/>
<connect gate="G$1" pin="A19" pad="17"/>
<connect gate="G$1" pin="A2" pad="9"/>
<connect gate="G$1" pin="A20" pad="39"/>
<connect gate="G$1" pin="A3" pad="8"/>
<connect gate="G$1" pin="A4" pad="7"/>
<connect gate="G$1" pin="A5" pad="48"/>
<connect gate="G$1" pin="A6" pad="47"/>
<connect gate="G$1" pin="A7" pad="46"/>
<connect gate="G$1" pin="A8" pad="45"/>
<connect gate="G$1" pin="A9" pad="44"/>
<connect gate="G$1" pin="CE1" pad="13"/>
<connect gate="G$1" pin="CE2" pad="16"/>
<connect gate="G$1" pin="DNU" pad="40"/>
<connect gate="G$1" pin="GND@1" pad="5"/>
<connect gate="G$1" pin="GND@2" pad="26"/>
<connect gate="G$1" pin="GND@3" pad="32"/>
<connect gate="G$1" pin="GND@4" pad="41"/>
<connect gate="G$1" pin="GND@5" pad="53"/>
<connect gate="G$1" pin="I/O00" pad="22"/>
<connect gate="G$1" pin="I/O01" pad="24"/>
<connect gate="G$1" pin="I/O02" pad="31"/>
<connect gate="G$1" pin="I/O03" pad="33"/>
<connect gate="G$1" pin="I/O04" pad="49"/>
<connect gate="G$1" pin="I/O05" pad="51"/>
<connect gate="G$1" pin="I/O06" pad="4"/>
<connect gate="G$1" pin="I/O07" pad="6"/>
<connect gate="G$1" pin="OE" pad="42"/>
<connect gate="G$1" pin="WE" pad="15"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CY7C1069AV33B" prefix="IC">
<description>&lt;b&gt;2M x 8 Static RAM&lt;/b&gt;&lt;p&gt;
Source: CYPRESS cy7c1069av33_8.pdf</description>
<gates>
<gate name="G$1" symbol="2048KX8-FBGA60"/>
</gates>
<devices>
<device name="" package="FBGA60-8X20">
<connects>
<connect gate="G$1" pin="+3V@1" pad="D6"/>
<connect gate="G$1" pin="+3V@2" pad="E1"/>
<connect gate="G$1" pin="A0" pad="A3"/>
<connect gate="G$1" pin="A1" pad="A4"/>
<connect gate="G$1" pin="A10" pad="H4"/>
<connect gate="G$1" pin="A11" pad="H5"/>
<connect gate="G$1" pin="A12" pad="G3"/>
<connect gate="G$1" pin="A13" pad="G4"/>
<connect gate="G$1" pin="A14" pad="F3"/>
<connect gate="G$1" pin="A15" pad="F4"/>
<connect gate="G$1" pin="A16" pad="E4"/>
<connect gate="G$1" pin="A17" pad="D3"/>
<connect gate="G$1" pin="A18" pad="E3"/>
<connect gate="G$1" pin="A19" pad="H1"/>
<connect gate="G$1" pin="A2" pad="A5"/>
<connect gate="G$1" pin="A20" pad="H6"/>
<connect gate="G$1" pin="A3" pad="B3"/>
<connect gate="G$1" pin="A4" pad="B4"/>
<connect gate="G$1" pin="A5" pad="C3"/>
<connect gate="G$1" pin="A6" pad="C4"/>
<connect gate="G$1" pin="A7" pad="D4"/>
<connect gate="G$1" pin="A8" pad="H2"/>
<connect gate="G$1" pin="A9" pad="H3"/>
<connect gate="G$1" pin="CE1" pad="B5"/>
<connect gate="G$1" pin="CE2" pad="A6"/>
<connect gate="G$1" pin="DNU" pad="G2"/>
<connect gate="G$1" pin="GND@1" pad="D1"/>
<connect gate="G$1" pin="GND@2" pad="E6"/>
<connect gate="G$1" pin="I/O00" pad="C1"/>
<connect gate="G$1" pin="I/O01" pad="D2"/>
<connect gate="G$1" pin="I/O02" pad="E2"/>
<connect gate="G$1" pin="I/O03" pad="F1"/>
<connect gate="G$1" pin="I/O04" pad="C6"/>
<connect gate="G$1" pin="I/O05" pad="D5"/>
<connect gate="G$1" pin="I/O06" pad="E5"/>
<connect gate="G$1" pin="I/O07" pad="F6"/>
<connect gate="G$1" pin="OE" pad="A2"/>
<connect gate="G$1" pin="WE" pad="G5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
