<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;MITSUBISHI SEMICONDUCTOR&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PS21962-ST">
<description>&lt;b&gt;DIPIPM 25&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.mitsubishichips.com/Global/content/product/powermod/powermod/dipipm/dipipmv4/ps21962-st_e.pdf"&gt; Data sheet&lt;/a&gt;</description>
</package>
<package name="SOP8">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt; 8P2S-A&lt;br&gt;
Plastic 8pin 225mil SOP&lt;br&gt;
Source: Mitsubishi M5218AL/P/FP</description>
</package>
</packages>
<symbols>
<symbol name="PS21962">
<pin name="VUFB" direction="in"/>
<pin name="VP1" direction="in"/>
<pin name="UP" direction="in"/>
<pin name="VNC" direction="in"/>
<pin name="VVFB" direction="in"/>
<pin name="VP" direction="in"/>
<pin name="VWFB" direction="in"/>
<pin name="WP" direction="in"/>
<pin name="VN1" direction="in"/>
<pin name="UN" direction="in"/>
<pin name="VN" direction="in"/>
<pin name="WN" direction="in"/>
<pin name="FO" direction="in"/>
<pin name="VNC@1" direction="in"/>
<pin name="CIN" direction="pas"/>
<pin name="NW" direction="out"/>
<pin name="NV" direction="out"/>
<pin name="NU" direction="out"/>
<pin name="W" direction="oc"/>
<pin name="V" direction="oc"/>
<pin name="U" direction="oc"/>
<pin name="P" direction="oc"/>
</symbol>
<symbol name="OPAMP">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="PS21962-ST" prefix="IC">
<description>&lt;b&gt;600V/5A low-loss 5th generation IGBT inverter bridge for three phase DC-to-AC power conversion&lt;/b&gt;&lt;p&gt;
Open emitter type&lt;br&gt;
Source: &lt;a href="http://www.mitsubishichips.com/Global/content/product/powermod/powermod/dipipm/dipipmv4/ps21962-st_e.pdf"&gt; Data sheet&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="PS21962"/>
</gates>
<devices>
<device name="" package="PS21962-ST">
<connects>
<connect gate="G$1" pin="CIN" pad="15"/>
<connect gate="G$1" pin="FO" pad="14"/>
<connect gate="G$1" pin="NU" pad="20"/>
<connect gate="G$1" pin="NV" pad="19"/>
<connect gate="G$1" pin="NW" pad="18"/>
<connect gate="G$1" pin="P" pad="24"/>
<connect gate="G$1" pin="U" pad="23"/>
<connect gate="G$1" pin="UN" pad="10"/>
<connect gate="G$1" pin="UP" pad="5"/>
<connect gate="G$1" pin="V" pad="22"/>
<connect gate="G$1" pin="VN" pad="11"/>
<connect gate="G$1" pin="VN1" pad="13"/>
<connect gate="G$1" pin="VNC" pad="9"/>
<connect gate="G$1" pin="VNC@1" pad="16"/>
<connect gate="G$1" pin="VP" pad="6"/>
<connect gate="G$1" pin="VP1" pad="8"/>
<connect gate="G$1" pin="VUFB" pad="2"/>
<connect gate="G$1" pin="VVFB" pad="3"/>
<connect gate="G$1" pin="VWFB" pad="4"/>
<connect gate="G$1" pin="W" pad="21"/>
<connect gate="G$1" pin="WN" pad="12"/>
<connect gate="G$1" pin="WP" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M5218" prefix="IC">
<description>&lt;b&gt;DUAL LOW-NOISE OPERATIONAL AMPLIFIER&lt;/b&gt; (DUAL POWER SUPPLY TYPE)&lt;p&gt;
Source: Mitsubishi M5218AL/P/FP</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="AFP" package="SOP8">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="V+" pad="8"/>
<connect gate="P" pin="V-" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
