<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<library>
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="E3206S">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, Eichhoff/distributor Schukat</description>
</package>
<package name="E3206L">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, Eichhoff/distributor Schukat</description>
</package>
<package name="SDS-S2">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
mono stable, 2 x norm. open, 2 x norm. closed, 5 A/250 V, AC/DC, NAiS</description>
</package>
<package name="SDS-ST2">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
polarity, 2 x norm. open, NAiS</description>
</package>
<package name="G6A-234P">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
</package>
<package name="G6A-434P">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
</package>
<package name="H550">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
bistable, 1 x switch, high current</description>
</package>
<package name="HE751">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open, Hamlin</description>
</package>
<package name="RP710">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Schrack</description>
</package>
<package name="RP420">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Schrack</description>
</package>
<package name="RP420A">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Schrack</description>
</package>
<package name="V23127A">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
horizontal, 1 x switch, 5 A/300 V DC, 250 V AC, Siemens</description>
</package>
<package name="MR24">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch</description>
</package>
<package name="351">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, same as G5 V-2, Omron</description>
</package>
<package name="DS2E-L2">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, 4 A/250 V, NAiS</description>
</package>
<package name="V23127B">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
vertical, 1 x switch, 5 A/300 V DC, 250 V AC, Siemens</description>
</package>
<package name="F4052">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Finder</description>
</package>
<package name="G6C-1117P">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, 10 A/240 V, Omron</description>
</package>
<package name="G6C-2117P">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, 1x norm. closed, 10 A/240 V, Omron</description>
</package>
<package name="G5LE">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, 10 A/120 V AC, 8 A/30 V ADC, Omron</description>
</package>
<package name="G6H2-100">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch 0.5 A/125 V AC, 1 A/30 V DC, Omron</description>
</package>
<package name="ZF112">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch</description>
</package>
<package name="RR1A">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, polarity, 1 x norm. open with shield</description>
</package>
<package name="RR1U">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, polarity, 1 x switch with shield</description>
</package>
<package name="RR2A">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, polarity, 2 x norm. open</description>
</package>
<package name="LY20">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Omron</description>
</package>
<package name="LY30">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
3 x switch, Omron</description>
</package>
<package name="LY40">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, Omron</description>
</package>
<package name="LY40S">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, Omron</description>
</package>
<package name="LY40SO">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x norm. open, Omron</description>
</package>
<package name="G2R">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, Omron</description>
</package>
<package name="G2RA">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, Omron</description>
</package>
<package name="G2R2">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Omron</description>
</package>
<package name="G2R2A">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x norm. open, Omron</description>
</package>
<package name="G2RE">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, high current, Omron</description>
</package>
<package name="G2REA">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, high current, Omron</description>
</package>
<package name="M3XXH">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch</description>
</package>
<package name="G5Y-1">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
RF up to 900 MHz, 1 x switch, 10 W, Omron</description>
</package>
<package name="FSMR">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, same as FBR21D/H, Fujitsu</description>
</package>
<package name="FRS1B">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, same as V23101-D6-A201, Siemens</description>
</package>
<package name="G6RW">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, Omron</description>
</package>
<package name="G6RS">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, Omron</description>
</package>
<package name="HE3321">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open, 7.62 mm, grid 5.08, Hamlin</description>
</package>
<package name="HE3621">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open, grid 5.08 mm, Hamlin</description>
</package>
<package name="HE3621S">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open with shield, grid 5.08 mm, Hamlin</description>
</package>
<package name="REED">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open with polarity, grid 5.08</description>
</package>
<package name="G5V1">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, 0.5 A/125 V AC, 1 A/24 V DC , Omron</description>
</package>
<package name="NA">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
dummy</description>
</package>
<package name="NAL">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
dummy long</description>
</package>
<package name="MT_78_603">
<description>&lt;b&gt;Relay socket MT 78 603&lt;/b&gt; SCHRACK&lt;p&gt;
Socket 11 pole with PCB terminals&lt;br&gt;
Source: http://www.schrack.com/.. 5932.pdf</description>
</package>
<package name="MT_78_602">
<description>&lt;b&gt;Relay socket MT 78 602&lt;/b&gt; SCHRACK&lt;p&gt;
Socket 8 pole with PCB terminals&lt;br&gt;
Source: http://www.schrack.com/.. 5932.pdf</description>
</package>
<package name="G6K-RF">
<description>&lt;b&gt;OMRON High Frequency Relay G6K-RF&lt;/b&gt;&lt;p&gt;
D20G6KRF0602.pdf</description>
</package>
<package name="G6KU-2P-Y">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="G6K-2F">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="G6K-2P">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="G6K-2F-Y">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="G6K-2G-Y">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="G6K-2G">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="G6K-2P-Y">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="G6KU-2F-Y">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="G6KU-2G-Y">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
</package>
<package name="V23148-CO">
<description>&lt;b&gt;Power PCB Relay U/UB close/open&lt;/b&gt;&lt;p&gt;
tyco/electronics; 1 pole 7 A, mono or bistabile&lt;br&gt;
www.schrackrelays.com/pdf/UUB.pdf</description>
</package>
<package name="V23148-NO">
<description>&lt;b&gt;Power PCB Relay U/UB normal open&lt;/b&gt;&lt;p&gt;
tyco/electronics; 1 pole 7 A, mono or bistabile&lt;br&gt;
www.schrackrelays.com/pdf/UUB.pdf</description>
</package>
<package name="V23148-NC">
<description>&lt;b&gt;Power PCB Relay U/UB normal close&lt;/b&gt;&lt;p&gt;
tyco/electronics; 1 pole 7 A, mono or bistabile&lt;br&gt;
www.schrackrelays.com/pdf/UUB.pdf</description>
</package>
<package name="G6AK-434P">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, dual coil latching, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
</package>
<package name="G6AU-434P">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, single coil latching, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
</package>
<package name="V23040201">
<description>&lt;b&gt;SIEMENS Mono- or Bisatil relay&lt;/b&gt;</description>
</package>
<package name="NAIS-LOGO">
<description>&lt;b&gt;NAiS&lt;/b&gt; Logo 6mm</description>
</package>
<package name="SSOP4">
<description>&lt;b&gt;SSOP 04&lt;/b&gt; NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="DIL04SMD">
<description>&lt;b&gt;DIL04 SMD&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="DIL06SMD">
<description>&lt;b&gt;DIL06 SMD&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="DIL08SMD">
<description>&lt;b&gt;DIL08&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="SOP04">
<description>&lt;b&gt;SOP 04 - 4.3x4.4mm RM 2.54mm&lt;/b&gt; AQY21, AQY22, AQY61 Series NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="SOP06">
<description>&lt;b&gt;SOP6 - AQV21, AQV22, AQV41&lt;/b&gt; Sereis NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="SOP08">
<description>&lt;b&gt;SOP 08 - AQW21, AQW61&lt;/b&gt; Series NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="SOP12">
<description>&lt;b&gt;AOP 12- AQW21.T2s&lt;/b&gt; Series NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="SOP16">
<description>&lt;b&gt;SOP 16 - AQS21, AQS22, AQS610TS&lt;/b&gt; Series NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="SIL13">
<description>&lt;b&gt;SIL 13 - AQX21.44&lt;/b&gt; Series (Multi-channel)&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="AQY27-SMD04">
<description>&lt;b&gt;SMD 04 9.4x8.8mm RM 5.08mm&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="AQW27-SMD08">
<description>&lt;b&gt;SMD 08&lt;/b&gt; NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="AQW27-DIL08">
<description>&lt;b&gt;DIL 08&lt;/b&gt; NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="AQZ-SIL04">
<description>&lt;b&gt;SIL 04&lt;/b&gt; NAiS&lt;p&gt;
Source: www.panasonic-electric-works.com .. photomos_sil4.dxf</description>
</package>
<package name="AQZ26-SIL04">
<description>&lt;b&gt;SIL 04&lt;/b&gt; NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="VS05-NAIS">
<description>&lt;b&gt;VS Modul&lt;/b&gt; NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  en_ds_61702_0000.pdf</description>
</package>
<package name="DIL07">
<description>&lt;b&gt;DIL07&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61613_0000.pdf</description>
</package>
<package name="DIL07SMD">
<description>&lt;b&gt;DIL07&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61613_0000.pdf</description>
</package>
<package name="DR-2">
<description>&lt;b&gt;DR Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: www.mew-europe.com/ac/download/ datasheet/relay/dr_en.pdf</description>
</package>
<package name="DR-1">
<description>&lt;b&gt;DR Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: www.mew-europe.com/ac/download/ datasheet/relay/dr_en.pdf</description>
</package>
<package name="AQG">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  en_ds_61611_0000.pdf</description>
</package>
<package name="AQE">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61610_0000.pdf</description>
</package>
<package name="HC2-PS-K">
<description>&lt;b&gt;Relay Socked&lt;/b&gt; NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  en_ds_61606_0000.pdf</description>
</package>
<package name="AQ-B">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61604_0000.pdf</description>
</package>
<package name="DIL04">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL06">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="AQZ404-PS">
<description>&lt;b&gt;Socked&lt;/b&gt; standard type PA1a-PS&lt;p&gt;
POWER PhotoMOS RELAYS 1-channel (Form B) Type&lt;br&gt;
Source: http://www.mew-europe.com/..  ds_aqz404.pdf</description>
</package>
<package name="AQZ404-PS-H">
<description>&lt;b&gt;Socked&lt;/b&gt; self clinching type PA1a-PS-H&lt;p&gt;
POWER PhotoMOS RELAYS 1-channel (Form B) Type&lt;br&gt;
Source: http://www.mew-europe.com/..  ds_aqz404.pdf</description>
</package>
<package name="REED-SERIES-A">
<description>&lt;b&gt;Single in line reed relay series A&lt;/b&gt;&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61001_0000.pdf</description>
</package>
<package name="DF2">
<description>&lt;b&gt;HIGHLY SENSITIVE DIP MINIATURE RELAY&lt;/b&gt;&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61002_0000.pdf</description>
</package>
<package name="DF2-L2">
<description>&lt;b&gt;HIGHLY SENSITIVE DIP MINIATURE RELAY&lt;/b&gt; 2 coil&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61002_0000.pdf</description>
</package>
<package name="DS1E">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS&lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
</package>
<package name="DS1E-L">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS&lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
</package>
<package name="DS2E">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS&lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
</package>
<package name="DS2E-L">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS&lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
</package>
<package name="DS4E">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt;&lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
</package>
<package name="DS4E-L">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt;&lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
</package>
<package name="DS-BT">
<description>&lt;b&gt;DS-BT RELAYS 4,000 V BREAKDOWN VOLTAGE&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0010.pdf</description>
</package>
<package name="DS2Y">
<description>&lt;b&gt;MINIATURE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0023.pdf</description>
</package>
<package name="DS2Y-2">
<description>&lt;b&gt;MINIATURE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0023.pdf</description>
</package>
<package name="GN">
<description>&lt;b&gt;ULTRA-SMALL PACKAGE SLIM POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61007_0000.pdf</description>
</package>
<package name="GN-A">
<description>&lt;b&gt;ULTRA-SMALL PACKAGE SLIM POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61007_0000.pdf</description>
</package>
<package name="GN-S">
<description>&lt;b&gt;ULTRA-SMALL PACKAGE SLIM POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61007_0000.pdf</description>
</package>
<package name="GQ">
<description>&lt;b&gt;ULTRA-SMALL PACKAGE FLAT POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61008_0000.pdf</description>
</package>
<package name="GQ-A">
<description>&lt;b&gt;ULTRA-SMALL PACKAGE FLAT POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61008_0000.pdf</description>
</package>
<package name="GQ-S">
<description>&lt;b&gt;ULTRA-SMALL PACKAGE FLAT POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61008_0000.pdf</description>
</package>
<package name="HX">
<description>&lt;b&gt;Compact &amp; Slim 2 Form C Non-polarized Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61011_0000.pdf</description>
</package>
<package name="HY">
<description>&lt;b&gt;Non-polarized 1 Form C Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61012_0000.pdf</description>
</package>
<package name="K2EBP">
<description>&lt;b&gt;UNIQUELY DESIGNED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61013_0000.pdf</description>
</package>
<package name="K4EBP">
<description>&lt;b&gt;UNIQUELY DESIGNED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61013_0000.pdf</description>
</package>
<package name="K6-PS">
<description>&lt;b&gt;RELAY Socked&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61013_0000.pdf</description>
</package>
<package name="K4-PS">
<description>&lt;b&gt;RELAY Socked&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61013_0000.pdf</description>
</package>
<package name="K2-PS">
<description>&lt;b&gt;RELAY Socked&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61013_0000.pdf</description>
</package>
<package name="NF2">
<description>&lt;b&gt;FLATPACK RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61014_0000.pdf</description>
</package>
<package name="NF4">
<description>&lt;b&gt;FLATPACK RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61014_0000.pdf</description>
</package>
<package name="NL6EBX">
<description>&lt;b&gt;6PDT FLATPACK 2AMP DIL RELAY&lt;/b&gt; NAiS&lt;p&gt;
Single side stable&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61014_0003.pdf</description>
</package>
<package name="NL6EBX-L2">
<description>&lt;b&gt;6PDT FLATPACK 2AMP DIL RELAY&lt;/b&gt; NAiS&lt;p&gt;
2 coil latching&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61014_0003.pdf</description>
</package>
<package name="TF2">
<description>&lt;b&gt;SMALL POLARIZED RELAY WITH HIGH SENSITIVITY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61017_0000.pdf</description>
</package>
<package name="TK">
<description>&lt;b&gt;ULTRA LOW PROFILE 2 AMP. POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61018_0000.pdf</description>
</package>
<package name="TN2">
<description>&lt;b&gt;SLIM POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61019_0000.pdf</description>
</package>
<package name="TQ2">
<description>&lt;b&gt;LOW PROFILE 2 FORM C RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61020_0001.pdf</description>
</package>
<package name="TQ4">
<description>&lt;b&gt;LOW PROFILE 2 FORM C RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61020_0001.pdf</description>
</package>
<package name="TQ-SA">
<description>&lt;b&gt;LOW-PROFILE TQ-SMD RELAYS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61021_0004.pdf</description>
</package>
<package name="TQ-SL">
<description>&lt;b&gt;LOW-PROFILE TQ-SMD RELAYS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61021_0004.pdf</description>
</package>
<package name="TQ-SS">
<description>&lt;b&gt;LOW-PROFILE TQ-SMD RELAYS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61021_0004.pdf</description>
</package>
<package name="TX2">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
</package>
<package name="TX2SL">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
</package>
<package name="TX2SA">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
</package>
<package name="TX2SS">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;
WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
</package>
<package name="TX2-L2">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;2 coil latching&lt;br&gt;Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
</package>
<package name="TX2SA-L2">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;2 coil latching&lt;br&gt;Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
</package>
<package name="TX2SL-L2">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;2 coil latching&lt;br&gt;Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
</package>
<package name="TX2SS-L2">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;
WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;
2 coil latching&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
</package>
<package name="TXD2">
<description>&lt;b&gt;HIGH INSULATION RELAYS&lt;/b&gt; NAiS&lt;p&gt;
Conforming to the supplementary insulation class of EN Standards (EN41003)&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0007.pdf</description>
</package>
<package name="TXD2SA">
<description>&lt;b&gt;HIGH INSULATION RELAYS&lt;/b&gt; NAiS&lt;p&gt;
Conforming to the supplementary insulation class of EN Standards (EN41003)&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0007.pdf</description>
</package>
<package name="TXD2SL">
<description>&lt;b&gt;HIGH INSULATION RELAYS&lt;/b&gt; NAiS&lt;p&gt;
Conforming to the supplementary insulation class of EN Standards (EN41003)&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0007.pdf</description>
</package>
<package name="TXD2SS">
<description>&lt;b&gt;HIGH INSULATION RELAYS&lt;/b&gt; NAiS&lt;p&gt;
Conforming to the supplementary insulation class of EN Standards (EN41003)&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0007.pdf</description>
</package>
<package name="LD">
<description>&lt;b&gt;Slim Power Relay&lt;/br&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61112_0000.pdf</description>
</package>
<package name="PE-FORM-A">
<description>&lt;b&gt;SLIM POWER Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61122_0000.pdf</description>
</package>
<package name="PE-FORM-C">
<description>&lt;b&gt;SLIM POWER Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61122_0000.pdf</description>
</package>
<package name="PE-SOCKET">
<description>&lt;b&gt;SLIM POWER Relay SOCKET&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61122_0000.pdf</description>
</package>
<package name="PA">
<description>&lt;b&gt;SLIM POWER RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61123_0000.pdf</description>
</package>
<package name="PA-STD-SOCKET">
<description>&lt;b&gt;SLIM POWER Relay SOCKET Standard&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61123_0000.pdf</description>
</package>
<package name="PA-CLI-SOCKET">
<description>&lt;b&gt;SLIM POWER Relay self clinching SOCKET&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61123_0000.pdf</description>
</package>
<package name="CB1">
<description>&lt;b&gt;HIGH POWER AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61202_0000.pdf</description>
</package>
<package name="CF">
<description>&lt;b&gt;NEW DUAL POWER AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61203_0000.pdf</description>
</package>
<package name="CM">
<description>&lt;b&gt;AUTOMOTIVE MICRO-ISO RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61204_0000.pdf</description>
</package>
<package name="CT-TWIN">
<description>&lt;b&gt;ULTRA SMALL AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Twin type (8 terminals)&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61205_0000.pdf</description>
</package>
<package name="CT-SLIM">
<description>&lt;b&gt;ULTRA SMALL AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Slim 1c type &lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61205_0000.pdf</description>
</package>
<package name="CT2-TWIN">
<description>&lt;b&gt;ULTRA SMALL AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Twin type (10 terminals)&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61205_0000.pdf</description>
</package>
<package name="CP1A">
<description>&lt;b&gt;ULTRA-MINIATURE LOW PROFILE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61207_0000.pdf</description>
</package>
<package name="CP1SA">
<description>&lt;b&gt;ULTRA-MINIATURE LOW PROFILE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61207_0000.pdf</description>
</package>
<package name="CP1">
<description>&lt;b&gt;ULTRA-MINIATURE LOW PROFILE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61207_0000.pdf</description>
</package>
<package name="CQ1">
<description>&lt;b&gt;AUTOMOTIVE QUIET RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61208_0000.pdf</description>
</package>
<package name="CR2">
<description>&lt;b&gt;DUAL POWER QUIET AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61209_0000.pdf</description>
</package>
<package name="JJM1A">
<description>&lt;b&gt;HALF-SIZE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61210_0001.pdf</description>
</package>
<package name="JJM1C">
<description>&lt;b&gt;HALF-SIZE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61210_0001.pdf</description>
</package>
<package name="JJM">
<description>&lt;b&gt;DOUBLE MAKE CONTACT AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61210_0002.pdf</description>
</package>
<package name="JS-M">
<description>&lt;b&gt;Automotive Ultra-Miniature Power Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61211_0000.pdf</description>
</package>
<package name="JS-M1A">
<description>&lt;b&gt;Automotive Ultra-Miniature Power Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61211_0000.pdf</description>
</package>
<package name="JT">
<description>&lt;b&gt;COMPACT ECONOMICAL 30 AMP. RELAY&lt;/b&gt; NAiS&lt;p&gt;
Open type&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61212_0000.pdf</description>
</package>
<package name="JT-PCB">
<description>&lt;b&gt;COMPACT ECONOMICAL 30 AMP. RELAY&lt;/b&gt; NAiS&lt;p&gt;
PCB type&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61212_0000.pdf</description>
</package>
<package name="JT-TMB">
<description>&lt;b&gt;COMPACT ECONOMICAL 30 AMP. RELAY&lt;/b&gt; NAiS&lt;p&gt;
TMB type&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61212_0000.pdf</description>
</package>
<package name="JT1A-TMB">
<description>&lt;b&gt;COMPACT ECONOMICAL 30 AMP. RELAY&lt;/b&gt; NAiS&lt;p&gt;
TMB type&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61212_0000.pdf</description>
</package>
<package name="JT1A">
<description>&lt;b&gt;COMPACT ECONOMICAL 30 AMP. RELAY&lt;/b&gt; NAiS&lt;p&gt;
Open type&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61212_0000.pdf</description>
</package>
<package name="JT1A-PCB">
<description>&lt;b&gt;COMPACT ECONOMICAL 30 AMP. RELAY&lt;/b&gt; NAiS&lt;p&gt;
PCB type&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61212_0000.pdf</description>
</package>
<package name="CV-MIRO-280">
<description>&lt;b&gt;AUTOMOTIVE LOW PROFILE MICRO-280 RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61214_0000.pdf</description>
</package>
<package name="CV1A-MICRO-280">
<description>&lt;b&gt;AUTOMOTIVE LOW PROFILE MICRO-280 RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61214_0000.pdf</description>
</package>
<package name="RG1">
<description>&lt;b&gt;HIGH FREQUENCY RELAYS WITH 1C AND 2C CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61302_0000.pdf</description>
</package>
<package name="RG2">
<description>&lt;b&gt;HIGH FREQUENCY RELAYS WITH 1C AND 2C CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61302_0000.pdf</description>
</package>
<package name="RM2">
<description>&lt;b&gt;4 GHz 2 FORM C MICROWAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61305_0000.pdf</description>
</package>
<package name="RM">
<description>&lt;b&gt;4 GHz 2 FORM C MICROWAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61305_0000.pdf</description>
</package>
<package name="RP">
<description>&lt;b&gt;LOW PROFILE HIGH FREQUENCY RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61306_0000.pdf</description>
</package>
<package name="RX2">
<description>&lt;b&gt;SMALL MICRO WAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61307_0000.pdf</description>
</package>
<package name="RX">
<description>&lt;b&gt;SMALL MICRO WAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61307_0000.pdf</description>
</package>
<package name="RA-2COIL">
<description>&lt;b&gt;MICROWAVE RELAY FOR ATTENUATOR CIRCUIT&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61308_0000.pdf</description>
</package>
<package name="RA-1COIL">
<description>&lt;b&gt;MICROWAVE RELAY FOR ATTENUATOR CIRCUIT&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61308_0000.pdf</description>
</package>
<package name="RA">
<description>&lt;b&gt;MICROWAVE RELAY FOR ATTENUATOR CIRCUIT&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61308_0000.pdf</description>
</package>
<package name="RE">
<description>&lt;b&gt;SMALL MICROWAVE RELAYS FOR BROADCASTING INDUSTRY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61310_0000.pdf</description>
</package>
<package name="RE-SMD">
<description>&lt;b&gt;SMALL MICROWAVE RELAYS FOR BROADCASTING INDUSTRY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61310_0000.pdf</description>
</package>
<package name="RK1A">
<description>&lt;b&gt;1.5 GHz MICROWAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61311_0000.pdf</description>
</package>
<package name="RKL2">
<description>&lt;b&gt;1.5 GHz MICROWAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61311_0000.pdf</description>
</package>
<package name="AQ1">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61601_0000.pdf</description>
</package>
<package name="AQ1-FLAT">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61601_0000.pdf</description>
</package>
<package name="AQ1-M">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61601_0000.pdf</description>
</package>
<package name="AQ-HS-5A">
<description>&lt;b&gt;Heat sink (for AC output, 5A type)&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61601_0000.pdf</description>
</package>
<package name="RJ">
<description>&lt;b&gt;SMD RELAYS WITH 5GHz CAPABILITIES&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61313_0000.pdf</description>
</package>
<package name="RJ-SMD">
<description>&lt;b&gt;SMD RELAYS WITH 5GHz CAPABILITIES&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61313_0000.pdf</description>
</package>
<package name="SF2">
<description>&lt;b&gt;POLARISED, MONOSTABLE RELAY WITH FORCIBLY GUIDED CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61404_0001.pdf&lt;br&gt;
&lt;a href="http://www.panasonic-electric-works.com/catalogues/downloads/relays/en_ds_61404_0001.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="SF4D">
<description>&lt;b&gt;POLARISED, MONOSTABLE RELAY WITH FORCIBLY GUIDED DOUBLE CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61407_0002.pdf</description>
</package>
<package name="S102T0X">
<description>&lt;b&gt;Low Height Type Solid State Relays&lt;/b&gt; SHARP&lt;p&gt;
Source: 162574-da-01-en-S202T02_Solid_State_Relais.pdf</description>
</package>
<package name="S2XXEX">
<description>&lt;b&gt;SIP Type SSR for Medium Power Control&lt;/b&gt; SHARP&lt;p&gt;
Source: 168149-da-01-en-Solid_State_Relais_S_202_SE1_SE2.pdf</description>
</package>
<package name="PE">
<description>&lt;b&gt;Miniature PCB Relay 1 pole 5 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5807.pdf</description>
</package>
<package name="SR2Y">
<description>&lt;b&gt;Safety Relay 2 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5809.pdf</description>
</package>
<package name="SR2X">
<description>&lt;b&gt;Safety Relay 2 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5807.pdf</description>
</package>
<package name="RE-SCHRACK">
<description>&lt;b&gt;Miniature PCB Relay 1 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5812.pdf</description>
</package>
<package name="SR6-D">
<description>&lt;b&gt;Safety Relay 4 pole 8 A&lt;/b&gt; SCHRACK&lt;p&gt;
2 N/O contact and 2 N/C contact&lt;br&gt;
Source: http://www.schrack.com/.. 5814.pdf</description>
</package>
<package name="SR6-M">
<description>&lt;b&gt;Safety Relay 4 pole 8 A&lt;/b&gt; SCHRACK&lt;p&gt;
Configuration 3 N/O contact and 1 N/C contact&lt;br&gt;
Source: http://www.schrack.com/.. 5814.pdf</description>
</package>
<package name="SNR-V">
<description>&lt;b&gt;Slim PCB Relay 1 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5815.pdf</description>
</package>
<package name="SNR-H">
<description>&lt;b&gt;Slim PCB Relay 1 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5815.pdf</description>
</package>
<package name="SNR-H6">
<description>&lt;b&gt;Slim PCB Relay 1 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5815.pdf</description>
</package>
<package name="SNR-V1">
<description>&lt;b&gt;Slim PCB Relay 1 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5815.pdf</description>
</package>
<package name="RY-II">
<description>&lt;b&gt;Miniature Power PCB Relay 1 pole 8 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5817.pdf</description>
</package>
<package name="RY-II1">
<description>&lt;b&gt;Miniature Power PCB Relay 1 pole 8 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5817.pdf</description>
</package>
<package name="RT-C/O16A5">
<description>&lt;b&gt;Power PCB Relay 1 pole 12 / 16 A, DC- or AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
16 A, pinning 5mm&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
</package>
<package name="RT-C/O12A3.5">
<description>&lt;b&gt;Power PCB Relay 1 pole 12 / 16 A, DC- or AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
12A, pinning 3.5 mm&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
</package>
<package name="RT-C/O12A5">
<description>&lt;b&gt;Power PCB Relay 1 pole 12 / 16 A, DC- or AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
12 A, pinning 5mm&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
</package>
<package name="RT-N/O16A5">
<description>&lt;b&gt;Power PCB Relay 1 pole 12 / 16 A, DC- or AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
16 A, pinning 5mm&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
</package>
<package name="RT-N/O12A5">
<description>&lt;b&gt;Power PCB Relay 1 pole 12 / 16 A, DC- or AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
12 A, pinning 5mm&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
</package>
<package name="RT-N/O12A3.5">
<description>&lt;b&gt;Power PCB Relay 1 pole 12 / 16 A, DC- or AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
12A, pinning 3.5 mm&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
</package>
<package name="RT1-BI">
<description>&lt;b&gt;Power PCB Relay , polarized bistable version&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A, pinning 5mm&lt;br&gt;
Source: http://www.schrack.com/.. 5821.pdf</description>
</package>
<package name="PT-4">
<description>&lt;b&gt;Miniature Relay&lt;/b&gt; SCHRACK&lt;p&gt;
4 pole 6 A DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5823.pdf</description>
</package>
<package name="PT-3">
<description>&lt;b&gt;Miniature Relay&lt;/b&gt; SCHRACK&lt;p&gt;
3 pole 10 A DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5823.pdf</description>
</package>
<package name="PT-2">
<description>&lt;b&gt;Miniature Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 12 A DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5823.pdf</description>
</package>
<package name="RM-2/3/7">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 / 3 pole 10 / 16 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5829.pdf</description>
</package>
<package name="RM-2">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 16 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5829.pdf</description>
</package>
<package name="RM-5">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
3 pole 10 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5832.pdf</description>
</package>
<package name="RM-6">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 16 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5832.pdf</description>
</package>
<package name="PT78604">
<description>&lt;b&gt;Accessories Miniature Relay PT&lt;/b&gt; SCHRACK&lt;p&gt;
Socket with PCB terminals 4 Pol.&lt;br&gt;
Source: http://www.schrack.com/.. 5836.pdf</description>
</package>
<package name="PT78602">
<description>&lt;b&gt;Accessories Miniature Relay PT&lt;/b&gt; SCHRACK&lt;p&gt;
Socket with PCB terminals 2 Pol.&lt;br&gt;
Source: http://www.schrack.com/.. 5836.pdf</description>
</package>
<package name="PT78603">
<description>&lt;b&gt;Accessories Miniature Relay PT&lt;/b&gt; SCHRACK&lt;p&gt;
Socket with PCB terminals 3 Pol.&lt;br&gt;
Source: http://www.schrack.com/.. 5836.pdf</description>
</package>
<package name="RP-SLF">
<description>&lt;b&gt;Special Load PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A, for high inrush currents, bistable&lt;br&gt;
Source: http://www.schrack.com/.. 5837.pdf</description>
</package>
<package name="RP-SLA">
<description>&lt;b&gt;Special Load PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A, for high inrush currents, monostable&lt;br&gt;
Source: http://www.schrack.com/.. 5837.pdf</description>
</package>
<package name="RPH">
<description>&lt;b&gt;Faston Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A&lt;br&gt;
Source: http://www.schrack.com/.. 5840.pdf</description>
</package>
<package name="RM78702">
<description>&lt;b&gt;Power Relay Socket with PCB terminals&lt;/b&gt; SCHRACK&lt;p&gt;
3 pole 10 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5841.pdf</description>
</package>
<package name="RT2N/O">
<description>&lt;b&gt;Power PCB Relay DC and AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5842.pdf</description>
</package>
<package name="RT2C/O">
<description>&lt;b&gt;Power PCB Relay DC and AC-coil&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5842.pdf</description>
</package>
<package name="RT424">
<description>&lt;b&gt;Power PCB Relay polarized bistable version&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5843.pdf</description>
</package>
<package name="RP440">
<description>&lt;b&gt;Power PCB Relay RP II/2&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5844.pdf</description>
</package>
<package name="RP61">
<description>&lt;b&gt;Power PCB Relay RP I&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A Horizontal version&lt;br&gt;
Source: http://www.schrack.com/.. 5845.pdf</description>
</package>
<package name="RP51">
<description>&lt;b&gt;Power PCB Relay RP I&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A Vertical version&lt;br&gt;
Source: http://www.schrack.com/.. 5845.pdf</description>
</package>
<package name="RP63">
<description>&lt;b&gt;Power PCB Relay RP I&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A Horizontal version&lt;br&gt;
Source: http://www.schrack.com/.. 5845.pdf</description>
</package>
<package name="RP53">
<description>&lt;b&gt;Power PCB Relay RP I&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A Vertical version&lt;br&gt;
Source: http://www.schrack.com/.. 5845.pdf</description>
</package>
<package name="PB">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1pole 10 A&lt;br&gt;
Source: http://www.schrack.com/.. 5846.pdf</description>
</package>
<package name="ZN5">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1pole 10 A&lt;br&gt;
Source: http://www.schrack.com/.. 5847.pdf</description>
</package>
<package name="ZN1">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1pole 10 A&lt;br&gt;
Source: http://www.schrack.com/.. 5847.pdf</description>
</package>
<package name="ZD1">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 30 A&lt;br&gt;
Source: http://www.schrack.com/.. 5848.pdf</description>
</package>
<package name="ZD2">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 30 A&lt;br&gt;
Source: http://www.schrack.com/.. 5848.pdf</description>
</package>
<package name="ZD2F">
<description>&lt;b&gt;Power Relay PCB-/Faston version&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 30 A&lt;br&gt;
Source: http://www.schrack.com/.. 5848.pdf</description>
</package>
<package name="ZD1F">
<description>&lt;b&gt;Power Relay PCB-/Faston version&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 30 A&lt;br&gt;
Source: http://www.schrack.com/.. 5848.pdf</description>
</package>
<package name="SR4">
<description>&lt;b&gt;Safety Relay&lt;/b&gt; SCHRACK&lt;p&gt;
4 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 6685.pdf</description>
</package>
<package name="SR6A">
<description>&lt;b&gt;Safety Relay SR6&lt;/b&gt; SCHRACK&lt;p&gt;
sensitive 6 pole 8 A, Type A and B&lt;br&gt;
Source: http://www.schrack.com/.. 6688.pdf</description>
</package>
<package name="SR6C">
<description>&lt;b&gt;Safety Relay SR6&lt;/b&gt; SCHRACK&lt;p&gt;
sensitive 6 pole 8 A, Type C&lt;br&gt;
Source: http://www.schrack.com/.. 6688.pdf</description>
</package>
<package name="SR6B">
<description>&lt;b&gt;Safety Relay SR6&lt;/b&gt; SCHRACK&lt;p&gt;
sensitive 6 pole 8 A, Type A&lt;br&gt;
Source: http://www.schrack.com/.. 6688.pdf</description>
</package>
<package name="AQY27">
<description>&lt;b&gt;DIL 04&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
<package name="NV2R">
<description>&lt;b&gt;MOTORUMPOL RELAIS 12V&lt;/b&gt;&lt;p&gt;
Ningbo Forward Relay Corporation LTD.&lt;br&gt;
Ningbo.Huaguan Electronics Corporation LTD.&lt;p&gt;
Source: http://www.dblectro.com/site/pdf/NV2R.pdf&lt;p&gt;
http://www2.produktinfo.conrad.com/datenblaetter/500000-524999/505013-da-01-de-Motorumpolrelais_12V.pdf&lt;br&gt;
Elli-Echo ER20T-S-DC12V - 20A/14VDC&lt;br&gt;
Conrad Nr.: 505013 - 62</description>
</package>
<package name="G6D">
<description>&lt;b&gt;Slim, Miniature Relay&lt;/b&gt; 17.5 × 6.5 × 12.5 mm&lt;p&gt;
Source: http://ecb.omron.com.sg/pdf/relay/power/G6D.pdf</description>
</package>
<package name="G6D-SOCKET">
<description>Slim, Miniature Relay &lt;b&gt;SOCKET&lt;/b&gt; 17.5 × 6.5 × 12.5 mm&lt;p&gt;
Source: http://ecb.omron.com.sg/pdf/relay/power/G6D.pdf</description>
</package>
<package name="G5SB">
<description>&lt;b&gt;Compact Single-pole Relay for Switching 5 A&lt;/b&gt;&lt;p&gt;
Source: http://www.omron.com/ecb/products/pry/121/g5sb.html</description>
</package>
<package name="S202S02">
<description>&lt;b&gt;S202S02&lt;/b&gt;&lt;p&gt;
Source: http://sharp-world.com/products/device/lineup/data/pdf/datasheet/s102s02_e.pdf</description>
</package>
<package name="G6J-2P-Y">
<description>&lt;b&gt;Signal Relay - G6J-Y&lt;/b&gt; 5.7 x 10.6 x 9 mm&lt;p&gt;
Source: http://www.omroncomponents.eu/ .. K125-E2-02-X.pdf</description>
</package>
<package name="G6J-2FS-Y">
<description>&lt;b&gt;Signal Relay - G6J-Y&lt;/b&gt; 5.7 x 10.6 x 9 mm&lt;p&gt;
Source: http://www.omroncomponents.eu/ .. K125-E2-02-X.pdf</description>
</package>
<package name="G6J-2FL-Y">
<description>&lt;b&gt;Signal Relay - G6J-Y&lt;/b&gt; 5.7 x 10.6 x 9 mm&lt;p&gt;
Source: http://www.omroncomponents.eu/ .. K125-E2-02-X.pdf</description>
</package>
<package name="CLARE002">
</package>
<package name="S102S01">
<description>&lt;b&gt;SHARP Solid State Relaiys&lt;/b&gt; IT(rms) 8A, Non-Zero Cross type&lt;p&gt;
Source: http://www.sharp.co.jp/products/device/lineup/data/pdf/datasheet/s102s01_j.pdf</description>
</package>
<package name="G5V-2">
<description>&lt;b&gt;OMRON PCB Relay&lt;/b&gt;&lt;p&gt;
Source: http://www.omron.com/ecb/products/pdf/en-g5v2.pdf</description>
</package>
<package name="BT-XX-S">
<description>&lt;ULTRA MINIATUR RELAY&lt;/b&gt;
Bestar Electric Ltd.&lt;br&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/500000-524999/505226-da-01-en-Kleinrelais_waschdicht_24V.pdf</description>
</package>
<package name="FTR-K1C">
<description>&lt;b&gt;Miniatur-Leistungsrelais&lt;/b&gt; 1 Wechsler&lt;p&gt;
Distributor: Conrad Electronic&lt;br&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/500000-524999/504389-da-01-de-NETZRELAIS_FTR-K1CK024W1XUM_16A_250VAC.pdf</description>
</package>
<package name="FTR-K1A">
<description>&lt;b&gt;Miniatur-Leistungsrelais&lt;/b&gt; 1 Schliesser&lt;p&gt;
Distributor: Conrad Electronic&lt;br&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/500000-524999/504389-da-01-de-NETZRELAIS_FTR-K1CK024W1XUM_16A_250VAC.pdf</description>
</package>
<package name="FTR-LYC">
<description>&lt;b&gt;Schmales Netzrelais&lt;/b&gt;&lt;p&gt;
Distributor: Conrad electronic&lt;br&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/500000-524999/504382-da-01-de-NETZRELAIS_FTR-LYCA024V_1XUM_6A_250VAC.pdf</description>
</package>
<package name="FINDER-30.22">
<description>&lt;b&gt;30 Series - Subminiature DIL relays 2 A&lt;/b&gt; Finder&lt;p&gt;
Source: http://www.farnell.com/datasheets/87634.pdf</description>
</package>
<package name="FINDER-43.41">
<description>&lt;b&gt; Low profile PCB relays 10 - 16 A&lt;/b&gt; FINDER - 43 Series&lt;p&gt;
Distributor: Farnell&lt;br&gt;
Source: http://www.farnell.com/datasheets/87682.pdf</description>
</package>
<package name="FINDER-43.61">
<description>&lt;b&gt;Low profile PCB relays 10 - 16 A&lt;/b&gt; FINDER 43 Series&lt;p&gt;
Kontakt max. AC- 250V,  Strom - Kontakt  AC- max. 10A&lt;br&gt;
5 mm contact pin pitch,  1 Pole NO, 16 A, PCB mount&lt;br&gt;
Distributor: FARNELL&lt;br&gt;
Source: http://www.farnell.com/datasheets/87682.pdf</description>
</package>
<package name="AZ8">
<description>&lt;b&gt;MINIATURE PC BOARD RELAY&lt;/b&gt;&lt;p&gt;
Source: www.azettler.com .. AZ8-1ch-12DSE.PDF</description>
</package>
<package name="9802-00">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt; Gull Wing&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
</package>
<package name="9802-20">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt; J-Lead&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
</package>
<package name="9814-00">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt; Gull Wing&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
</package>
<package name="9814-20">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt; J-Lead&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
</package>
<package name="9852-00">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt; Gull Wing&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
</package>
<package name="9852-20">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt; J-Lead&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
</package>
<package name="6561-0300">
<description>&lt;b&gt;20 / 30 A-Leistungsrelais&lt;/b&gt;&lt;p&gt;
Source: http://www.finder.de/comuni/pdf/S65DE.pdf</description>
</package>
<package name="I4-PAC">
<description>&lt;b&gt;Single-Pole, Normally Open i4-PAC (TM)&lt;/b&gt; DC Power Relay&lt;p&gt;
Source: &lt;a href="http://www.clare.com/home/pdfs.nsf/www/CPC1708.pdf/$file/CPC1708.pdf"&gt; Data sheet &lt;/a&gt;&lt;br&gt;</description>
</package>
<package name="FTR-B4S">
<description>&lt;b&gt;ULTRA MINIATURE RELAY 2 POLES - 2 A&lt;/b&gt; (Slim Profile Signal Relay)&lt;p&gt;
FUJITSU FTR-B4 SERIES&lt;br&gt;
Source: FTR-B4.pdf</description>
</package>
<package name="FTR-B4G">
<description>&lt;b&gt;ULTRA MINIATURE RELAY 2 POLES - 2 A&lt;/b&gt; (Slim Profile Signal Relay)&lt;p&gt;
FUJITSU FTR-B4 SERIES&lt;br&gt;
Source: FTR-B4.pdf</description>
</package>
<package name="FTR-B4C">
<description>&lt;b&gt;ULTRA MINIATURE RELAY 2 POLES - 2 A&lt;/b&gt; (Slim Profile Signal Relay)&lt;p&gt;
FUJITSU FTR-B4 SERIES&lt;br&gt;
Source: FTR-B4.pdf</description>
</package>
<package name="JW1A">
<description>&lt;b&gt;Power relay&lt;/b&gt;&lt;p&gt;
Source: Panasonic Electric Works Co., Ltd. / jw.catalog.pdf</description>
</package>
<package name="JW1C">
<description>&lt;b&gt;Power relay&lt;/b&gt;&lt;p&gt;
Source: Panasonic Electric Works Co., Ltd. / jw.catalog.pdf</description>
</package>
<package name="JW2A">
<description>&lt;b&gt;Power relay&lt;/b&gt;&lt;p&gt;
Source: Panasonic Electric Works Co., Ltd. / jw.catalog.pdf</description>
</package>
<package name="JW2C">
<description>&lt;b&gt;Power relay&lt;/b&gt;&lt;p&gt;
Source: Panasonic Electric Works Co., Ltd. / jw.catalog.pdf</description>
</package>
<package name="JV-KT">
<description>&lt;b&gt;POWER RELAY JV SERIES&lt;/b&gt; 1 POLE—5 A (MEDIUM LOAD CONTROL)&lt;p&gt;
Source: &lt;a href="http://www.produktinfo.conrad.com/datenblaetter/500000-524999/502946-da-01-en-RELAIS_JV_12S_KT.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="APF30212A">
<description>&lt;b&gt;Compliant with European standards 1a/1c 6A Slim power relays&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://pewa.panasonic.com/assets/pcsd/catalog/pf-catalog.pdf"&gt;Data sheet &lt;/a&gt;</description>
</package>
<package name="APF30212C">
<description>&lt;b&gt;Compliant with European standards 1a/1c 6A Slim power relays&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://pewa.panasonic.com/assets/pcsd/catalog/pf-catalog.pdf"&gt;Data sheet &lt;/a&gt;</description>
</package>
</packages>
<symbols>
<symbol name="K">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="KD">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="U">
<pin name="O" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="P" direction="pas"/>
</symbol>
<symbol name="KD-A">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="S">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="UD">
<pin name="O@1" direction="pas"/>
<pin name="S@1" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="P@1" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="K2">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="O">
<pin name="P" direction="pas"/>
<pin name="O" direction="pas"/>
</symbol>
<symbol name="SD">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="P@1" direction="pas"/>
<pin name="S@1" direction="pas"/>
</symbol>
<symbol name="U1">
<pin name="O" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="P@1" direction="pas"/>
</symbol>
<symbol name="U_M4">
<pin name="O" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="ES@1" direction="pas"/>
<pin name="ES@2" direction="pas"/>
<pin name="ES@3" direction="pas"/>
<pin name="ES@4" direction="pas"/>
</symbol>
<symbol name="S_M2">
<pin name="S" direction="pas"/>
<pin name="P" direction="pas"/>
<pin name="ES@1" direction="pas"/>
<pin name="ES@2" direction="pas"/>
</symbol>
<symbol name="K+-D">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="K+-">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="K-D-SIL">
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="S-SIL">
<pin name="S" direction="pas"/>
<pin name="P" direction="pas"/>
</symbol>
<symbol name="SHIELD">
<pin name="SH" direction="pas"/>
</symbol>
<symbol name="K+-S-+R">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="K+-S">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="K+-R">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="2304201">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="UV">
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="KV">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="PHOTOMOS_2D">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
<symbol name="DS_AQS210PS">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="PHOTOMOS-DC">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
<symbol name="PHOTOMOS-DC3">
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
<symbol name="AQS">
<pin name="K" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="K1" direction="pas"/>
<pin name="D3" direction="pas"/>
<pin name="D4" direction="pas"/>
<pin name="A1" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="PHOTO-RELAY-2S">
<pin name="K" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="PHOTO-DETECTOR">
<pin name="K" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="AC2" direction="pas"/>
<pin name="AC1" direction="pas"/>
</symbol>
<symbol name="PHOTO-REKAY2D1S">
<pin name="K" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PHOTO-REKAY-2LED-2D1S">
<pin name="K" direction="pas"/>
<pin name="D1" direction="pas"/>
<pin name="D2" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PHOTOMOS_2D_NO">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
<symbol name="PHOTOMOS_2D_NC">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
<symbol name="AQZ20OV">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
<symbol name="VS-MODUL">
<pin name="L1" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="+" direction="pas"/>
<pin name="L2" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="PHOTOTRIAC">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
<symbol name="PHOTOTRIAC-Z">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
<symbol name="PHOTOTRIAC-2Z">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
<pin name="DS3" direction="pas"/>
<pin name="K1" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="PHOTOTRIAC-2">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
<pin name="DS3" direction="pas"/>
<pin name="K1" direction="pas"/>
<pin name="K2" direction="pas"/>
</symbol>
<symbol name="+KS+KR-">
<pin name="-" direction="pas"/>
<pin name="R+" direction="pas"/>
<pin name="S+" direction="pas"/>
</symbol>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
<symbol name="CF">
<pin name="NC" direction="pas"/>
<pin name="NO" direction="pas"/>
<pin name="COM1" direction="pas"/>
<pin name="COM2" direction="pas"/>
</symbol>
<symbol name="K2-1">
<pin name="M" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="S2">
<pin name="C" direction="pas"/>
<pin name="NO1" direction="pas"/>
<pin name="NO2" direction="pas"/>
</symbol>
<symbol name="K-DIODE">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
<symbol name="SHIELD-4">
<pin name="SH@3" direction="pas"/>
<pin name="SH@1" direction="pas"/>
<pin name="SH@2" direction="pas"/>
<pin name="SH@4" direction="pas"/>
</symbol>
<symbol name="K-PIN">
<pin name="-" direction="pas"/>
</symbol>
<symbol name="SHIELD-3">
<pin name="SH@2" direction="pas"/>
<pin name="SH@3" direction="pas"/>
<pin name="SH@1" direction="pas"/>
</symbol>
<symbol name="SHIELD-2">
<pin name="SH@2" direction="pas"/>
<pin name="SH@1" direction="pas"/>
</symbol>
<symbol name="U-X2">
<pin name="OA" direction="pas"/>
<pin name="SA" direction="pas"/>
<pin name="PA" direction="pas"/>
<pin name="SB" direction="pas"/>
<pin name="OB" direction="pas"/>
<pin name="PB" direction="pas"/>
</symbol>
<symbol name="S-X2">
<pin name="PA" direction="pas"/>
<pin name="SA" direction="pas"/>
<pin name="SB" direction="pas"/>
<pin name="PB" direction="pas"/>
</symbol>
<symbol name="NV2R">
<pin name="A+" direction="pas"/>
<pin name="A" direction="pas"/>
<pin name="A-" direction="pas"/>
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
<pin name="B+" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="B-" direction="pas"/>
</symbol>
<symbol name="9802">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="9852">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="K-2P">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="1_" direction="pas"/>
<pin name="2_" direction="pas"/>
</symbol>
<symbol name="O-2P">
<pin name="P" direction="pas"/>
<pin name="O" direction="pas"/>
<pin name="O_" direction="pas"/>
<pin name="P_" direction="pas"/>
</symbol>
<symbol name="S-2P">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S_" direction="pas"/>
<pin name="P_" direction="pas"/>
</symbol>
<symbol name="PHOTOMOS_DC">
<pin name="A" direction="pas"/>
<pin name="K" direction="pas"/>
<pin name="DS1" direction="pas"/>
<pin name="DS2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="H550" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
bistable, 1 x switch, high current</description>
<gates>
<gate name="1" symbol="KD"/>
<gate name="2" symbol="UD"/>
</gates>
<devices>
<device name="" package="H550">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="3" pad="3"/>
<connect gate="2" pin="O" pad="O0"/>
<connect gate="2" pin="O@1" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="P@1" pad="P0"/>
<connect gate="2" pin="S" pad="S0"/>
<connect gate="2" pin="S@1" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="E3206L" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, Eichhoff/distributor Schukat</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="E3206L">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HE751" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open, Hamlin</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="HE751">
<connects>
<connect gate="1" pin="1" pad="2"/>
<connect gate="1" pin="2" pad="6"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP710" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Schrack</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="UD"/>
</gates>
<devices>
<device name="" package="RP710">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O0"/>
<connect gate="2" pin="O@1" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="P@1" pad="P0"/>
<connect gate="2" pin="S" pad="S0"/>
<connect gate="2" pin="S@1" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP710024"/>
<attribute name="OC_FARNELL" value="388312"/>
<attribute name="OC_NEWARK" value="17M1785"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP42?*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/2&lt;/b&gt; Schrack&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5844.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="0" package="RP420">
<connects>
<connect gate="1" pin="1" pad="A2"/>
<connect gate="1" pin="2" pad="A1"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP420005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7798"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP420006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7799"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP420012"/>
<attribute name="OC_FARNELL" value="3103330"/>
<attribute name="OC_NEWARK" value="90B4410"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP420024"/>
<attribute name="OC_FARNELL" value="1703720"/>
<attribute name="OC_NEWARK" value="51B969"/>
</technology>
<technology name="048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP420048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C3381"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP420060"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7803"/>
</technology>
<technology name="110">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP420110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3601"/>
</technology>
</technologies>
</device>
<device name="1" package="RP420">
<connects>
<connect gate="1" pin="1" pad="A2"/>
<connect gate="1" pin="2" pad="A1"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="6-1393234-4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H0760"/>
</technology>
<technology name="006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="6-1393234-5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H0761"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP421012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90B5481"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP421024"/>
<attribute name="OC_FARNELL" value="1608388"/>
<attribute name="OC_NEWARK" value="01C0518"/>
</technology>
<technology name="048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP421048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3604"/>
</technology>
<technology name="060">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP421060"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="84H0645"/>
</technology>
<technology name="110">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP421110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="39C2625"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V23127A" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
horizontal, 1 x switch, 5 A/300 V DC, 250 V AC, Siemens</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="V23127A">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V23127B" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
vertical, 1 x switch, 5 A/300 V DC, 250 V AC, Siemens</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="V23127B">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G5L" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, 10 A/120 V AC, 8 A/30 V ADC, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="G5LE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="351" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="351">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="16"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="4052" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Finder</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="F4052">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS2-L2-*" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt; NAiS &lt;p&gt;
bistable, 2 x switch, 4 A/250 V</description>
<gates>
<gate name="1" symbol="K2"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="DS2E-L2">
<connects>
<connect gate="1" pin="1" pad="16"/>
<connect gate="1" pin="2" pad="1"/>
<connect gate="1" pin="3" pad="2"/>
<connect gate="1" pin="4" pad="15"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="E3206S" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, Eichhoff/distributor Schukat</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="E3206S">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6A-234P" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="G6A-234P">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="16"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6A-434P" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
<gate name="5" symbol="U"/>
</gates>
<devices>
<device name="" package="G6A-434P">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="16"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
<connect gate="4" pin="O" pad="O3"/>
<connect gate="4" pin="P" pad="P3"/>
<connect gate="4" pin="S" pad="S3"/>
<connect gate="5" pin="O" pad="O4"/>
<connect gate="5" pin="P" pad="P4"/>
<connect gate="5" pin="S" pad="S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6C-1117P" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, 10 A/240 V, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="G6C-1117P">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="8"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6C-2117P" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, 1x norm. closed, 10 A/240 V, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="O"/>
</gates>
<devices>
<device name="" package="G6C-2117P">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="8"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="S2"/>
<connect gate="3" pin="P" pad="P2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6H2-100" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, 0.5 A/125 V AC, 1 A/30 V DC, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="G6H2-100">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="10"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDS-S2" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
monostable, 2 x norm. open, 2 x norm. closed, 5 A/250 V AC/DC, NAiS</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="5" symbol="S"/>
<gate name="3" symbol="S"/>
<gate name="2" symbol="O"/>
<gate name="4" symbol="O"/>
</gates>
<devices>
<device name="" package="SDS-S2">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="12"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
<connect gate="4" pin="O" pad="O3"/>
<connect gate="4" pin="P" pad="P3"/>
<connect gate="5" pin="P" pad="P4"/>
<connect gate="5" pin="S" pad="S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SDS-ST2" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
polarity, 2 x norm. open, NAiS</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
</gates>
<devices>
<device name="" package="SDS-ST2">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="4"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZF112" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="ZF112">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RR1A" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, polarity, 1 x norm. open with shield</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="SD"/>
</gates>
<devices>
<device name="" package="RR1A">
<connects>
<connect gate="1" pin="1" pad="2"/>
<connect gate="1" pin="2" pad="6"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="P@1" pad="8"/>
<connect gate="2" pin="S" pad="1"/>
<connect gate="2" pin="S@1" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RR1U" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, polarity, 1 x switch with shield</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U1"/>
</gates>
<devices>
<device name="" package="RR1U">
<connects>
<connect gate="1" pin="1" pad="2"/>
<connect gate="1" pin="2" pad="6"/>
<connect gate="2" pin="O" pad="1"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="P@1" pad="8"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RR2A" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, polarity, 2 x norm. open</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
</gates>
<devices>
<device name="" package="RR2A">
<connects>
<connect gate="1" pin="1" pad="2"/>
<connect gate="1" pin="2" pad="6"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="1"/>
<connect gate="3" pin="P" pad="8"/>
<connect gate="3" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LY20" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="LY20">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LY30" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
3 x switch, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="LY30">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
<connect gate="4" pin="O" pad="O3"/>
<connect gate="4" pin="P" pad="P3"/>
<connect gate="4" pin="S" pad="S3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LY40" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
<gate name="5" symbol="U"/>
</gates>
<devices>
<device name="" package="LY40">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
<connect gate="4" pin="O" pad="O3"/>
<connect gate="4" pin="P" pad="P3"/>
<connect gate="4" pin="S" pad="S3"/>
<connect gate="5" pin="O" pad="O4"/>
<connect gate="5" pin="P" pad="P4"/>
<connect gate="5" pin="S" pad="S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LY40S" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="S"/>
</gates>
<devices>
<device name="" package="LY40S">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
<connect gate="4" pin="P" pad="P3"/>
<connect gate="4" pin="S" pad="S3"/>
<connect gate="5" pin="P" pad="P4"/>
<connect gate="5" pin="S" pad="S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G2R" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="G2R">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1569185"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G2R2" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x switch, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="G2R2">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G2R-2-DC6"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89C5317"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G2R2A" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
2 x norm. open, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
</gates>
<devices>
<device name="" package="G2R2A">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="G2R-2A-DC24"/>
<attribute name="OC_FARNELL" value="6985269"/>
<attribute name="OC_NEWARK" value="36M5257"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G2RA" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="G2RA">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G2RE" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, high current, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="UD"/>
</gates>
<devices>
<device name="" package="G2RE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O0"/>
<connect gate="2" pin="O@1" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="P@1" pad="P0"/>
<connect gate="2" pin="S" pad="S0"/>
<connect gate="2" pin="S@1" pad="S1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G2REA" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, high current, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="SD"/>
</gates>
<devices>
<device name="" package="G2REA">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="P@1" pad="P@"/>
<connect gate="2" pin="S" pad="S"/>
<connect gate="2" pin="S@1" pad="S@"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="M3XXH" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U1"/>
</gates>
<devices>
<device name="" package="M3XXH">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="P@1" pad="P@"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G5Y-1" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
RF Relay up to 900 MHz, 1 x switch, 10 W, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U_M4"/>
</gates>
<devices>
<device name="" package="G5Y-1">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="7"/>
<connect gate="2" pin="ES@1" pad="9"/>
<connect gate="2" pin="ES@2" pad="10"/>
<connect gate="2" pin="ES@3" pad="12"/>
<connect gate="2" pin="ES@4" pad="13"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRS1B" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, same as V23101-D6-A201, Siemens</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U1"/>
</gates>
<devices>
<device name="" package="FRS1B">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="P@1" pad="P@"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FSMR" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, same as FBR21D/H, Fujitsu</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U1"/>
</gates>
<devices>
<device name="" package="FSMR">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="P@1" pad="P@"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6RW" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="G6RW">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6RS" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x norm. open, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="G6RS">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HE3321" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open, 7.62 mm, grid 5.08 mm, Hamlin</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="HE3321">
<connects>
<connect gate="1" pin="1" pad="2"/>
<connect gate="1" pin="2" pad="3"/>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="S" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="HAMLIN"/>
<attribute name="MPN" value="HE3321C1200"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="46F3928"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HE3621" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open, grid 5.08 mm, Hamlin</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="HE3621">
<connects>
<connect gate="1" pin="+" pad="2"/>
<connect gate="1" pin="-" pad="3"/>
<connect gate="2" pin="P" pad="4"/>
<connect gate="2" pin="S" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="HAMLIN"/>
<attribute name="MPN" value="HE3621A2410"/>
<attribute name="OC_FARNELL" value="9561943"/>
<attribute name="OC_NEWARK" value="50F7993"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HE3621S" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open with shield, grid 5.08 mm, Hamlin</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="S_M2"/>
</gates>
<devices>
<device name="" package="HE3621S">
<connects>
<connect gate="1" pin="+" pad="2"/>
<connect gate="1" pin="-" pad="3"/>
<connect gate="2" pin="ES@1" pad="5"/>
<connect gate="2" pin="ES@2" pad="6"/>
<connect gate="2" pin="P" pad="4"/>
<connect gate="2" pin="S" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MR24" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
<gate name="5" symbol="U"/>
</gates>
<devices>
<device name="" package="MR24">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O1"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="O" pad="O2"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
<connect gate="4" pin="O" pad="O3"/>
<connect gate="4" pin="P" pad="P3"/>
<connect gate="4" pin="S" pad="S3"/>
<connect gate="5" pin="O" pad="O4"/>
<connect gate="5" pin="P" pad="P4"/>
<connect gate="5" pin="S" pad="S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="35701331" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open with polarity</description>
<gates>
<gate name="1" symbol="K-D-SIL"/>
<gate name="2" symbol="S-SIL"/>
</gates>
<devices>
<device name="" package="REED">
<connects>
<connect gate="1" pin="3" pad="3"/>
<connect gate="1" pin="5" pad="5"/>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="S" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G5V1" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, 0.5 A/125 V AC, 1 A/24 V DC , Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U1"/>
</gates>
<devices>
<device name="" package="G5V1">
<connects>
<connect gate="1" pin="1" pad="2"/>
<connect gate="1" pin="2" pad="9"/>
<connect gate="2" pin="O" pad="1"/>
<connect gate="2" pin="P" pad="5"/>
<connect gate="2" pin="P@1" pad="6"/>
<connect gate="2" pin="S" pad="10"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="G5V-1-DC24"/>
<attribute name="OC_FARNELL" value="9949593"/>
<attribute name="OC_NEWARK" value="36M6377"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NA" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="NA">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="12"/>
<connect gate="2" pin="O" pad="3"/>
<connect gate="2" pin="P" pad="4"/>
<connect gate="2" pin="S" pad="5"/>
<connect gate="3" pin="O" pad="10"/>
<connect gate="3" pin="P" pad="9"/>
<connect gate="3" pin="S" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NAL" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="K+-"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="NAL">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="12"/>
<connect gate="2" pin="+" pad="6"/>
<connect gate="2" pin="-" pad="7"/>
<connect gate="3" pin="O" pad="3"/>
<connect gate="3" pin="P" pad="4"/>
<connect gate="3" pin="S" pad="5"/>
<connect gate="4" pin="O" pad="10"/>
<connect gate="4" pin="P" pad="9"/>
<connect gate="4" pin="S" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G5LE" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, 10 A/120 V AC, 8 A/30 V DC, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="G5LE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="O"/>
<connect gate="2" pin="P" pad="P"/>
<connect gate="2" pin="S" pad="S"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LY40SO" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x norm. open, Omron</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="S"/>
</gates>
<devices>
<device name="" package="LY40SO">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="P1"/>
<connect gate="2" pin="S" pad="S1"/>
<connect gate="3" pin="P" pad="P2"/>
<connect gate="3" pin="S" pad="S2"/>
<connect gate="4" pin="P" pad="P3"/>
<connect gate="4" pin="S" pad="S3"/>
<connect gate="5" pin="P" pad="P4"/>
<connect gate="5" pin="S" pad="S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REED" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
reed, 1 x norm. open with polarity, grid 5.08</description>
<gates>
<gate name="2" symbol="S"/>
<gate name="1" symbol="K+-"/>
</gates>
<devices>
<device name="" package="REED">
<connects>
<connect gate="1" pin="+" pad="3"/>
<connect gate="1" pin="-" pad="5"/>
<connect gate="2" pin="P" pad="1"/>
<connect gate="2" pin="S" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6K*-2F-RF" prefix="K">
<description>&lt;b&gt;OMRON High Frequency Relay G6K-RF&lt;/b&gt;&lt;p&gt;
Compact High Frequency Relays with 2 Form C (DPDT) Contacts&lt;br&gt;
Handles 1 A, 30 VDC discrete load and 1 W at 1 GHz high frequency load&lt;br&gt;
D20G6KRF0602.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="A" symbol="U"/>
<gate name="B" symbol="U"/>
<gate name="S1" symbol="SHIELD"/>
<gate name="S2" symbol="SHIELD"/>
</gates>
<devices>
<device name="" package="G6K-RF">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="A" pin="O" pad="2"/>
<connect gate="A" pin="P" pad="3"/>
<connect gate="A" pin="S" pad="4"/>
<connect gate="B" pin="O" pad="7"/>
<connect gate="B" pin="P" pad="6"/>
<connect gate="B" pin="S" pad="5"/>
<connect gate="S1" pin="SH" pad="A"/>
<connect gate="S2" pin="SH" pad="B"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6K-2F-RF-DC12"/>
<attribute name="OC_FARNELL" value="1448181"/>
<attribute name="OC_NEWARK" value="73C8948"/>
</technology>
<technology name="U">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6K" prefix="K">
<description>&lt;b&gt;Low Signal Relay&lt;/b&gt;&lt;p&gt;
oeiwcsnts1.omron.com/.. D20G6K0100.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="-2F" package="G6K-2F">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6K-2F DC24"/>
<attribute name="OC_FARNELL" value="1690427"/>
<attribute name="OC_NEWARK" value="36K7467"/>
</technology>
</technologies>
</device>
<device name="-2G" package="G6K-2G">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6K-2G DC12"/>
<attribute name="OC_FARNELL" value="4601695"/>
<attribute name="OC_NEWARK" value="93B9118"/>
</technology>
</technologies>
</device>
<device name="-2P" package="G6K-2P">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6K-2P DC3"/>
<attribute name="OC_FARNELL" value="3937276"/>
<attribute name="OC_NEWARK" value="89C6482"/>
</technology>
</technologies>
</device>
<device name="-2F-Y" package="G6K-2F-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6K-2F-Y DC3"/>
<attribute name="OC_FARNELL" value="1690316"/>
<attribute name="OC_NEWARK" value="89C6451"/>
</technology>
</technologies>
</device>
<device name="-2G-Y" package="G6K-2G-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="4484794"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-2P-Y" package="G6K-2P-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6K-2P-Y DC12"/>
<attribute name="OC_FARNELL" value="3937276"/>
<attribute name="OC_NEWARK" value="34C3464"/>
</technology>
</technologies>
</device>
<device name="U-2F-Y" package="G6KU-2F-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6KU-2F-Y DC3"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89C6496"/>
</technology>
</technologies>
</device>
<device name="U-2G-Y" package="G6KU-2G-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6KU-2G-Y DC5"/>
<attribute name="OC_FARNELL" value="1690320"/>
<attribute name="OC_NEWARK" value="89C6505"/>
</technology>
</technologies>
</device>
<device name="U-2P-Y" package="G6KU-2P-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6KU-2P-Y DC5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="35K4536"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V23148-*-CO" prefix="K">
<description>&lt;b&gt;Power PCB Relay U/UB close/open&lt;/b&gt;&lt;p&gt;
tyco/electronics; 1 pole 7 A, mono or bistabile&lt;br&gt;
www.schrackrelays.com/pdf/UUB.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="V23148-CO">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="A0003-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1107-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="23M2638"/>
</technology>
<technology name="A0005-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1105-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="34M8971"/>
</technology>
<technology name="A0007-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1107-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="23M2638"/>
</technology>
<technology name="A0008-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1107-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="23M2638"/>
</technology>
<technology name="A0105-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1105-A101"/>
<attribute name="OC_FARNELL" value="1175042"/>
<attribute name="OC_NEWARK" value="34M8971"/>
</technology>
<technology name="A0107-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1107-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="23M2638"/>
</technology>
<technology name="A1005-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1105-A101"/>
<attribute name="OC_FARNELL" value="1175042"/>
<attribute name="OC_NEWARK" value="34M8971"/>
</technology>
<technology name="A1007-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1107-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="23M2638"/>
</technology>
<technology name="A1105-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1105-A101"/>
<attribute name="OC_FARNELL" value="1175042"/>
<attribute name="OC_NEWARK" value="34M8971"/>
</technology>
<technology name="A1107-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1107-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="23M2638"/>
</technology>
<technology name="B0003-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-B0005-A101"/>
<attribute name="OC_FARNELL" value="1175042"/>
<attribute name="OC_NEWARK" value="48M9081"/>
</technology>
<technology name="B0005-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-B0005-A101"/>
<attribute name="OC_FARNELL" value="1175042"/>
<attribute name="OC_NEWARK" value="48M9081"/>
</technology>
<technology name="B0007-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-B0008-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="16R7906"/>
</technology>
<technology name="B0008-A101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-B0008-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="16R7906"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V23148-*-NO" prefix="K">
<description>&lt;b&gt;Power PCB Relay U/UB normal open&lt;/b&gt;&lt;p&gt;
tyco/electronics;  1 pole 7 A, mono or bistabile&lt;br&gt;
www.schrackrelays.com/pdf/UUB.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="V23148-NO">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="A0003-B101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A0007-A101"/>
<attribute name="OC_FARNELL" value="1175042"/>
<attribute name="OC_NEWARK" value="48M9078"/>
</technology>
<technology name="A0005-B101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A1105-A101"/>
<attribute name="OC_FARNELL" value="1175042"/>
<attribute name="OC_NEWARK" value="34M8971"/>
</technology>
<technology name="A0007-B101">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23148-A0007-A101"/>
<attribute name="OC_FARNELL" value="1175043"/>
<attribute name="OC_NEWARK" value="48M9078"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6AK-434P" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, dual coil latching, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
<gates>
<gate name="-S" symbol="K+-S"/>
<gate name="-R" symbol="K+-R"/>
<gate name="-1" symbol="U"/>
<gate name="-2" symbol="U"/>
<gate name="-3" symbol="U"/>
<gate name="-4" symbol="U"/>
</gates>
<devices>
<device name="" package="G6AK-434P">
<connects>
<connect gate="-1" pin="O" pad="6"/>
<connect gate="-1" pin="P" pad="4"/>
<connect gate="-1" pin="S" pad="8"/>
<connect gate="-2" pin="O" pad="11"/>
<connect gate="-2" pin="P" pad="13"/>
<connect gate="-2" pin="S" pad="9"/>
<connect gate="-3" pin="O" pad="12"/>
<connect gate="-3" pin="P" pad="14"/>
<connect gate="-3" pin="S" pad="10"/>
<connect gate="-4" pin="O" pad="5"/>
<connect gate="-4" pin="P" pad="3"/>
<connect gate="-4" pin="S" pad="7"/>
<connect gate="-R" pin="+" pad="2"/>
<connect gate="-R" pin="-" pad="15"/>
<connect gate="-S" pin="+" pad="1"/>
<connect gate="-S" pin="-" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6AU-434P" prefix="K">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
4 x switch, single coil latching, 0.3 A/125 V AC, 1 A/30 V DC, Omron</description>
<gates>
<gate name="-RS" symbol="K+-S-+R"/>
<gate name="-1" symbol="U"/>
<gate name="-2" symbol="U"/>
<gate name="-3" symbol="U"/>
<gate name="-4" symbol="U"/>
</gates>
<devices>
<device name="" package="G6AU-434P">
<connects>
<connect gate="-1" pin="O" pad="6"/>
<connect gate="-1" pin="P" pad="4"/>
<connect gate="-1" pin="S" pad="8"/>
<connect gate="-2" pin="O" pad="11"/>
<connect gate="-2" pin="P" pad="13"/>
<connect gate="-2" pin="S" pad="9"/>
<connect gate="-3" pin="O" pad="12"/>
<connect gate="-3" pin="P" pad="14"/>
<connect gate="-3" pin="S" pad="10"/>
<connect gate="-4" pin="O" pad="5"/>
<connect gate="-4" pin="P" pad="3"/>
<connect gate="-4" pin="S" pad="7"/>
<connect gate="-RS" pin="+" pad="1"/>
<connect gate="-RS" pin="-" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V23040-*-B201" prefix="RL">
<description>&lt;b&gt;SIEMENS&lt;/b&gt;&lt;p&gt;
Monostabil A0001 = 5V; A0002 = 12V; A0003 = 15V; A0004 = 24V&lt;br&gt;
Bistabil C0051 = 5V; C0052 = 12V</description>
<gates>
<gate name="K" symbol="KV"/>
<gate name="K1" symbol="UV"/>
</gates>
<devices>
<device name="" package="V23040201">
<connects>
<connect gate="K" pin="1" pad="1"/>
<connect gate="K" pin="2" pad="2"/>
<connect gate="K" pin="3" pad="3"/>
<connect gate="K1" pin="4" pad="4"/>
<connect gate="K1" pin="5" pad="5"/>
<connect gate="K1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="A0001">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A0002">
<attribute name="MF" value=""/>
<attribute name="MPN" value="V23040-A0002-B201"/>
<attribute name="OC_FARNELL" value="1174994"/>
<attribute name="OC_NEWARK" value="24M9075"/>
</technology>
<technology name="A0003">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A0004">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQY221*2V" prefix="K">
<description>&lt;b&gt;PHOTOMOS Relay&lt;/b&gt; RF (Radio Frequency) NAiS&lt;p&gt;
C . R 10 SSOP Type;&lt;br&gt;
Source: http://www.mew-europe.com/.. aqy221_2v.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS_2D"/>
</gates>
<devices>
<device name="" package="SSOP4">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="DS1" pad="4"/>
<connect gate="G$1" pin="DS2" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name="N">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQY221N2V"/>
<attribute name="OC_FARNELL" value="1448344"/>
<attribute name="OC_NEWARK" value="13P1186"/>
</technology>
<technology name="R">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQY221R2V"/>
<attribute name="OC_FARNELL" value="1839014"/>
<attribute name="OC_NEWARK" value="94C1062"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQS210PS" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="DS_AQS210PS"/>
</gates>
<devices>
<device name="" package="SOP16">
<connects>
<connect gate="-1" pin="10" pad="10"/>
<connect gate="-1" pin="11" pad="11"/>
<connect gate="-1" pin="12" pad="12"/>
<connect gate="-1" pin="13" pad="13"/>
<connect gate="-1" pin="14" pad="14"/>
<connect gate="-1" pin="15" pad="15"/>
<connect gate="-1" pin="16" pad="16"/>
<connect gate="-1" pin="2" pad="2"/>
<connect gate="-1" pin="3" pad="3"/>
<connect gate="-1" pin="7" pad="7"/>
<connect gate="-1" pin="8" pad="8"/>
<connect gate="-1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQV*" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: &lt;a href="http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqv10_20.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="PHOTO-REKAY-2LED-2D1S"/>
</gates>
<devices>
<device name="" package="DIL06">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="D2" pad="4"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="10">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQV102"/>
<attribute name="OC_FARNELL" value="2006029"/>
<attribute name="OC_NEWARK" value="94F8718"/>
</technology>
<technology name="20">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQV201"/>
<attribute name="OC_FARNELL" value="1704180"/>
<attribute name="OC_NEWARK" value="50F4048"/>
</technology>
<technology name="21">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQV210"/>
<attribute name="OC_FARNELL" value="1704179"/>
<attribute name="OC_NEWARK" value="13P0968"/>
</technology>
<technology name="22">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1414197"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="23">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="234">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQV234"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1031"/>
</technology>
<technology name="25">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="41">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="45">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SMD" package="DIL06SMD">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="D2" pad="4"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="21">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQV210S"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="95F6433"/>
</technology>
<technology name="22">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="23">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="25">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SOP" package="SOP06">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="D2" pad="4"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="21">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="22">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="41">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQV254R" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTO-REKAY-2LED-2D1S"/>
</gates>
<devices>
<device name="" package="DIL06">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="D1" pad="6"/>
<connect gate="G$1" pin="D2" pad="4"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQV254"/>
<attribute name="OC_FARNELL" value="1124063"/>
<attribute name="OC_NEWARK" value="93F6300"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQW*" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="PHOTO-RELAY-2S"/>
<gate name="-2" symbol="PHOTO-RELAY-2S"/>
</gates>
<devices>
<device name="" package="DIL08">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="D1" pad="8"/>
<connect gate="-1" pin="D2" pad="7"/>
<connect gate="-1" pin="K" pad="2"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="D1" pad="6"/>
<connect gate="-2" pin="D2" pad="5"/>
<connect gate="-2" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="21">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="22">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="25">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="27">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="41">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="45">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="654">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQW654"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1160"/>
</technology>
</technologies>
</device>
<device name="SOP" package="SOP08">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="D1" pad="8"/>
<connect gate="-1" pin="D2" pad="7"/>
<connect gate="-1" pin="K" pad="2"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="D1" pad="6"/>
<connect gate="-2" pin="D2" pad="5"/>
<connect gate="-2" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="21">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SMD" package="DIL08SMD">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="D1" pad="8"/>
<connect gate="-1" pin="D2" pad="7"/>
<connect gate="-1" pin="K" pad="2"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="D1" pad="6"/>
<connect gate="-2" pin="D2" pad="5"/>
<connect gate="-2" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="654">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQW654"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="98B6279"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQW6*" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt; 
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="PHOTOMOS_2D_NC"/>
<gate name="-2" symbol="PHOTOMOS_2D_NO"/>
</gates>
<devices>
<device name="SOP" package="SOP08">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="DS1" pad="8"/>
<connect gate="-1" pin="DS2" pad="7"/>
<connect gate="-1" pin="K" pad="2"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="DS1" pad="6"/>
<connect gate="-2" pin="DS2" pad="5"/>
<connect gate="-2" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQW21OTS" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="PHOTOMOS_2D"/>
<gate name="-2" symbol="PHOTO-DETECTOR"/>
</gates>
<devices>
<device name="" package="SOP08">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="DS1" pad="8"/>
<connect gate="-1" pin="DS2" pad="7"/>
<connect gate="-1" pin="K" pad="2"/>
<connect gate="-2" pin="AC1" pad="6"/>
<connect gate="-2" pin="AC2" pad="5"/>
<connect gate="-2" pin="E" pad="4"/>
<connect gate="-2" pin="K" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQW21OT2S" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="PHOTOMOS_2D"/>
<gate name="-2" symbol="PHOTO-DETECTOR"/>
<gate name="-3" symbol="PHOTO-DETECTOR"/>
</gates>
<devices>
<device name="" package="SOP12">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="DS1" pad="12"/>
<connect gate="-1" pin="DS2" pad="11"/>
<connect gate="-1" pin="K" pad="2"/>
<connect gate="-2" pin="AC1" pad="10"/>
<connect gate="-2" pin="AC2" pad="9"/>
<connect gate="-2" pin="E" pad="4"/>
<connect gate="-2" pin="K" pad="3"/>
<connect gate="-3" pin="AC1" pad="8"/>
<connect gate="-3" pin="AC2" pad="7"/>
<connect gate="-3" pin="E" pad="6"/>
<connect gate="-3" pin="K" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQS210TS" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="PHOTO-REKAY2D1S"/>
<gate name="-2" symbol="PHOTO-REKAY2D1S"/>
<gate name="-3" symbol="PHOTO-DETECTOR"/>
</gates>
<devices>
<device name="" package="SOP16">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="D1" pad="16"/>
<connect gate="-1" pin="D2" pad="14"/>
<connect gate="-1" pin="K" pad="3"/>
<connect gate="-1" pin="S" pad="15"/>
<connect gate="-2" pin="A" pad="4"/>
<connect gate="-2" pin="D1" pad="13"/>
<connect gate="-2" pin="D2" pad="11"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-2" pin="S" pad="12"/>
<connect gate="-3" pin="AC1" pad="10"/>
<connect gate="-3" pin="AC2" pad="9"/>
<connect gate="-3" pin="E" pad="6"/>
<connect gate="-3" pin="K" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQS210T2S" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="PHOTO-REKAY2D1S"/>
<gate name="-2" symbol="PHOTO-DETECTOR"/>
<gate name="-3" symbol="PHOTO-DETECTOR"/>
</gates>
<devices>
<device name="" package="SOP16">
<connects>
<connect gate="-1" pin="A" pad="2"/>
<connect gate="-1" pin="D1" pad="16"/>
<connect gate="-1" pin="D2" pad="14"/>
<connect gate="-1" pin="K" pad="3"/>
<connect gate="-1" pin="S" pad="15"/>
<connect gate="-2" pin="AC1" pad="12"/>
<connect gate="-2" pin="AC2" pad="11"/>
<connect gate="-2" pin="E" pad="4"/>
<connect gate="-2" pin="K" pad="5"/>
<connect gate="-3" pin="AC1" pad="10"/>
<connect gate="-3" pin="AC2" pad="9"/>
<connect gate="-3" pin="E" pad="6"/>
<connect gate="-3" pin="K" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQS225S" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="PHOTOMOS_2D"/>
<gate name="-2" symbol="PHOTOMOS_2D"/>
<gate name="-3" symbol="PHOTOMOS_2D"/>
<gate name="-4" symbol="PHOTOMOS_2D"/>
</gates>
<devices>
<device name="" package="SOP16">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="DS1" pad="16"/>
<connect gate="-1" pin="DS2" pad="15"/>
<connect gate="-1" pin="K" pad="2"/>
<connect gate="-2" pin="A" pad="3"/>
<connect gate="-2" pin="DS1" pad="14"/>
<connect gate="-2" pin="DS2" pad="13"/>
<connect gate="-2" pin="K" pad="4"/>
<connect gate="-3" pin="A" pad="5"/>
<connect gate="-3" pin="DS1" pad="12"/>
<connect gate="-3" pin="DS2" pad="11"/>
<connect gate="-3" pin="K" pad="6"/>
<connect gate="-4" pin="A" pad="7"/>
<connect gate="-4" pin="DS1" pad="10"/>
<connect gate="-4" pin="DS2" pad="9"/>
<connect gate="-4" pin="K" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQS225S"/>
<attribute name="OC_FARNELL" value="1448339"/>
<attribute name="OC_NEWARK" value="10C3715"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQX21444" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  pti_en.pdf</description>
<gates>
<gate name="-1" symbol="PHOTOMOS_2D"/>
<gate name="-2" symbol="PHOTOMOS-DC3"/>
<gate name="-3" symbol="PHOTOMOS-DC3"/>
<gate name="-4" symbol="PHOTOMOS-DC3"/>
</gates>
<devices>
<device name="" package="SIL13">
<connects>
<connect gate="-1" pin="A" pad="1"/>
<connect gate="-1" pin="DS1" pad="6"/>
<connect gate="-1" pin="DS2" pad="7"/>
<connect gate="-1" pin="K" pad="2"/>
<connect gate="-2" pin="DS1" pad="8"/>
<connect gate="-2" pin="DS2" pad="9"/>
<connect gate="-2" pin="K" pad="3"/>
<connect gate="-3" pin="DS1" pad="10"/>
<connect gate="-3" pin="DS2" pad="11"/>
<connect gate="-3" pin="K" pad="4"/>
<connect gate="-4" pin="DS1" pad="12"/>
<connect gate="-4" pin="DS2" pad="13"/>
<connect gate="-4" pin="K" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQZ2*" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqz10_20.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS_2D"/>
</gates>
<devices>
<device name="" package="AQZ-SIL04">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="3"/>
<connect gate="G$1" pin="DS2" pad="4"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQZ*" prefix="K">
<description>&lt;b&gt;Power PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqz10_20.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS-DC"/>
</gates>
<devices>
<device name="" package="AQZ-SIL04">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="3"/>
<connect gate="G$1" pin="DS2" pad="4"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="102">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ102"/>
<attribute name="OC_FARNELL" value="1448345"/>
<attribute name="OC_NEWARK" value="52F5584"/>
</technology>
<technology name="104">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ104"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1217"/>
</technology>
<technology name="105">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ105"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1218"/>
</technology>
<technology name="107">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ107"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="50B844"/>
</technology>
<technology name="202">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ202"/>
<attribute name="OC_FARNELL" value="1175735"/>
<attribute name="OC_NEWARK" value="13P1220"/>
</technology>
<technology name="204">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ204"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1222"/>
</technology>
<technology name="205">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ205"/>
<attribute name="OC_FARNELL" value="1175736"/>
<attribute name="OC_NEWARK" value="13P1223"/>
</technology>
<technology name="207">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ207"/>
<attribute name="OC_FARNELL" value="1129299"/>
<attribute name="OC_NEWARK" value="64K3058"/>
</technology>
</technologies>
</device>
<device name="404-PS" package="AQZ404-PS">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="5"/>
<connect gate="G$1" pin="DS2" pad="6"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ404"/>
<attribute name="OC_FARNELL" value="1101853"/>
<attribute name="OC_NEWARK" value="13P1226"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQZ20OV" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqz10_20.pdf</description>
<gates>
<gate name="G$1" symbol="AQZ20OV"/>
</gates>
<devices>
<device name="" package="AQZ-SIL04">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="3"/>
<connect gate="G$1" pin="DS2" pad="4"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQZ20*D" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqz10_20.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS_2D"/>
</gates>
<devices>
<device name="" package="AQZ-SIL04">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="3"/>
<connect gate="G$1" pin="DS2" pad="4"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ202D"/>
<attribute name="OC_FARNELL" value="2053925"/>
<attribute name="OC_NEWARK" value="10C4043"/>
</technology>
<technology name="4">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ204D"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C4045"/>
</technology>
<technology name="5">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ205D"/>
<attribute name="OC_FARNELL" value="1175736"/>
<attribute name="OC_NEWARK" value="10C4047"/>
</technology>
<technology name="7">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ207"/>
<attribute name="OC_FARNELL" value="1129299"/>
<attribute name="OC_NEWARK" value="64K3058"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQZ10*D" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqz10_20.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS-DC"/>
</gates>
<devices>
<device name="" package="AQZ-SIL04">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="4"/>
<connect gate="G$1" pin="DS2" pad="3"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="2">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ102D"/>
<attribute name="OC_FARNELL" value="1448345"/>
<attribute name="OC_NEWARK" value="10C4038"/>
</technology>
<technology name="4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ104"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1217"/>
</technology>
<technology name="5">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ105"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C4041"/>
</technology>
<technology name="7">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQZ107"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="50B844"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQZ40" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqz10_20.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS_2D"/>
</gates>
<devices>
<device name="" package="AQZ-SIL04">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="4"/>
<connect gate="G$1" pin="DS2" pad="3"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="4-PS" package="AQZ404-PS">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="5"/>
<connect gate="G$1" pin="DS2" pad="6"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ404"/>
<attribute name="OC_FARNELL" value="1101853"/>
<attribute name="OC_NEWARK" value="13P1226"/>
</technology>
</technologies>
</device>
<device name="4-PS-H" package="AQZ404-PS-H">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="5"/>
<connect gate="G$1" pin="DS2" pad="6"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQZ404"/>
<attribute name="OC_FARNELL" value="1101853"/>
<attribute name="OC_NEWARK" value="13P1226"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQY*" prefix="K">
<description>&lt;b&gt;PhotoMOS Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqz10_20.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS_2D"/>
</gates>
<devices>
<device name="SOP" package="SOP04">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="DS1" pad="4"/>
<connect gate="G$1" pin="DS2" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name="21">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="22">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="41">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SMD" package="AQY27-SMD04">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="DS1" pad="4"/>
<connect gate="G$1" pin="DS2" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name="27">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="AQY27" package="AQY27">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="DS1" pad="4"/>
<connect gate="G$1" pin="DS2" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VS-MODUL" prefix="IC">
<description>&lt;b&gt;ELECTRONIC SWITCHING CIRCUIT&lt;/b&gt; NAiS&lt;p&gt;
Following Relais can combine to VS-Device:&lt;br&gt;
DE, DF, DK, DS, DSP, DX, R, RA, RG, RK, RM, RX, S, SP, ST, SX, TF, TN, TK, TQ, TQ-SA, TX&lt;br&gt;
Source: http://www.mew-europe.com/..&lt;br&gt;1060dlde0301.pdf&lt;br&gt;en_ds_61702_0000.pdf</description>
<gates>
<gate name="G$1" symbol="VS-MODUL"/>
</gates>
<devices>
<device name="" package="VS05-NAIS">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="5"/>
<connect gate="G$1" pin="K" pad="2"/>
<connect gate="G$1" pin="L1" pad="1"/>
<connect gate="G$1" pin="L2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATP1211S*" prefix="K">
<description>&lt;b&gt;Phototriac Coupler with Zero-Cross&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61690_0000.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOTRIAC-Z"/>
</gates>
<devices>
<device name="" package="SOP04">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="DS1" pad="4"/>
<connect gate="G$1" pin="DS2" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name="X">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Z">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ATP2121S*" prefix="K">
<description>&lt;b&gt;Phototriac Coupler&lt;/b&gt; none Zero-Cross NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61690_0000.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOTRIAC"/>
</gates>
<devices>
<device name="" package="SOP04">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="DS1" pad="4"/>
<connect gate="G$1" pin="DS2" pad="3"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name="X">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Z">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQH*213" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61613_0000.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOTRIAC-2Z"/>
</gates>
<devices>
<device name="" package="DIL07">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="8"/>
<connect gate="G$1" pin="DS2" pad="5"/>
<connect gate="G$1" pin="DS3" pad="6"/>
<connect gate="G$1" pin="K" pad="1"/>
<connect gate="G$1" pin="K1" pad="3"/>
<connect gate="G$1" pin="K2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="DIL07SMD">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="8"/>
<connect gate="G$1" pin="DS2" pad="5"/>
<connect gate="G$1" pin="DS3" pad="6"/>
<connect gate="G$1" pin="K" pad="1"/>
<connect gate="G$1" pin="K1" pad="3"/>
<connect gate="G$1" pin="K2" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQH*223" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61613_0000.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOTRIAC-2"/>
</gates>
<devices>
<device name="" package="DIL07">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="8"/>
<connect gate="G$1" pin="DS2" pad="5"/>
<connect gate="G$1" pin="DS3" pad="6"/>
<connect gate="G$1" pin="K" pad="1"/>
<connect gate="G$1" pin="K1" pad="3"/>
<connect gate="G$1" pin="K2" pad="4"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQH1223"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="54K4251"/>
</technology>
<technology name="2">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQH2223"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="26K3059"/>
</technology>
</technologies>
</device>
<device name="A" package="DIL07SMD">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="DS1" pad="8"/>
<connect gate="G$1" pin="DS2" pad="5"/>
<connect gate="G$1" pin="DS3" pad="6"/>
<connect gate="G$1" pin="K" pad="1"/>
<connect gate="G$1" pin="K1" pad="3"/>
<connect gate="G$1" pin="K2" pad="4"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQH1223A"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2601"/>
</technology>
<technology name="2">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQH2223A"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="26K3060"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DR-*V" prefix="K">
<description>&lt;b&gt;HIGHLY RELIABLE MINIATURE DIP RELAYS&lt;/b&gt; NAiS&lt;p&gt;
Source: www.mew-europe.com/ac/download/ datasheet/relay/dr_en.pdf</description>
<gates>
<gate name="-1" symbol="K+-"/>
<gate name="-2" symbol="U"/>
</gates>
<devices>
<device name="" package="DR-1">
<connects>
<connect gate="-1" pin="+" pad="3"/>
<connect gate="-1" pin="-" pad="14"/>
<connect gate="-2" pin="O" pad="1"/>
<connect gate="-2" pin="P" pad="8"/>
<connect gate="-2" pin="S" pad="16"/>
</connects>
<technologies>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DR-12V"/>
<attribute name="OC_FARNELL" value="1124066"/>
<attribute name="OC_NEWARK" value="91K6794"/>
</technology>
<technology name="15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DR-24V"/>
<attribute name="OC_FARNELL" value="1124068"/>
<attribute name="OC_NEWARK" value="21M8932"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DR-5V"/>
<attribute name="OC_FARNELL" value="1124065"/>
<attribute name="OC_NEWARK" value="24M1478"/>
</technology>
<technology name="C-12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="C-5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DR-L2-*V" prefix="K">
<description>&lt;b&gt;HIGHLY RELIABLE MINIATURE DIP RELAYS 2 Coil Latching&lt;/b&gt; NAiS&lt;p&gt;
Source: www.mew-europe.com/ac/download/datasheet/relay/dr_en.pdf</description>
<gates>
<gate name="C" symbol="U"/>
<gate name="A" symbol="K2"/>
</gates>
<devices>
<device name="" package="DR-2">
<connects>
<connect gate="A" pin="1" pad="3"/>
<connect gate="A" pin="2" pad="14"/>
<connect gate="A" pin="3" pad="6"/>
<connect gate="A" pin="4" pad="11"/>
<connect gate="C" pin="O" pad="16"/>
<connect gate="C" pin="P" pad="8"/>
<connect gate="C" pin="S" pad="1"/>
</connects>
<technologies>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQG*" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Zero-cross, Non zero-cross&lt;br&gt;
Source: http://www.mew-europe.com/.. en_ds_61611_0000.pdf</description>
<gates>
<gate name="A" symbol="PHOTOTRIAC"/>
</gates>
<devices>
<device name="" package="AQG">
<connects>
<connect gate="A" pin="A" pad="+"/>
<connect gate="A" pin="DS1" pad="O2"/>
<connect gate="A" pin="DS2" pad="O1"/>
<connect gate="A" pin="K" pad="-"/>
</connects>
<technologies>
<technology name="12105">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQG12105"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="20J4759"/>
</technology>
<technology name="12112">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG12112"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2581"/>
</technology>
<technology name="12124">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQG12124"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11J1737"/>
</technology>
<technology name="12205">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG12205"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2582"/>
</technology>
<technology name="12212">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG12212"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2583"/>
</technology>
<technology name="12224">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG12224"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2584"/>
</technology>
<technology name="22105">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG22105"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0946"/>
</technology>
<technology name="22110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="22124">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG22124"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2586"/>
</technology>
<technology name="22205">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG22205"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2587"/>
</technology>
<technology name="22212">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG22212"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2588"/>
</technology>
<technology name="22224">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQG22224"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2589"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQE*" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61610_0000.pdf</description>
<gates>
<gate name="A" symbol="PHOTOTRIAC"/>
</gates>
<devices>
<device name="" package="AQE">
<connects>
<connect gate="A" pin="A" pad="I+"/>
<connect gate="A" pin="DS1" pad="3+"/>
<connect gate="A" pin="DS2" pad="4-"/>
<connect gate="A" pin="K" pad="I-"/>
</connects>
<technologies>
<technology name="12105">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12112">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12124">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="34205">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="34212">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="34224">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQF*/AC" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61606_0000.pdf</description>
<gates>
<gate name="A" symbol="PHOTOTRIAC-Z"/>
</gates>
<devices>
<device name="" package="HC2-PS-K">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="DS1" pad="8"/>
<connect gate="A" pin="DS2" pad="12"/>
<connect gate="A" pin="K" pad="13"/>
</connects>
<technologies>
<technology name="2A2-ZT3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3A2-ZT3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQF*/DC" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61606_0000.pdf</description>
<gates>
<gate name="A" symbol="PHOTOMOS-DC"/>
</gates>
<devices>
<device name="" package="HC2-PS-K">
<connects>
<connect gate="A" pin="A" pad="14"/>
<connect gate="A" pin="DS1" pad="8"/>
<connect gate="A" pin="DS2" pad="12"/>
<connect gate="A" pin="K" pad="13"/>
</connects>
<technologies>
<technology name="2AD1-3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3AD1-3">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="REED-?-*" prefix="K">
<description>&lt;b&gt;Single in line reed relay series A&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61001_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="A" package="REED-SERIES-A">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="4"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="2"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF2-?DC*" prefix="K">
<description>&lt;b&gt;HIGHLY SENSITIVE DIP MINIATURE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Single side stable / 1 coil latching&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61002_0000.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="DF2">
<connects>
<connect gate="1" pin="+" pad="12"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="5"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="6"/>
<connect gate="3" pin="O" pad="8"/>
<connect gate="3" pin="P" pad="10"/>
<connect gate="3" pin="S" pad="7"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L-" package="DF2">
<connects>
<connect gate="1" pin="+" pad="12"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="5"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="6"/>
<connect gate="3" pin="O" pad="8"/>
<connect gate="3" pin="P" pad="10"/>
<connect gate="3" pin="S" pad="7"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DF2-L2-DC*" prefix="K">
<description>&lt;b&gt;HIGHLY SENSITIVE DIP MINIATURE RELAY&lt;/b&gt; NAiS&lt;p&gt;
2 coil latching Set/Reset&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61002_0000.pdf</description>
<gates>
<gate name="S" symbol="K+-"/>
<gate name="R" symbol="K+-"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="DF2-L2">
<connects>
<connect gate="3" pin="O" pad="5"/>
<connect gate="3" pin="P" pad="3"/>
<connect gate="3" pin="S" pad="6"/>
<connect gate="4" pin="O" pad="8"/>
<connect gate="4" pin="P" pad="10"/>
<connect gate="4" pin="S" pad="7"/>
<connect gate="R" pin="+" pad="11"/>
<connect gate="R" pin="-" pad="2"/>
<connect gate="S" pin="+" pad="12"/>
<connect gate="S" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1E-*?" prefix="K">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS &lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
<gates>
<gate name="2" symbol="U"/>
<gate name="1" symbol="K+-"/>
</gates>
<devices>
<device name="" package="DS1E">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="6"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L-" package="DS1E">
<connects>
<connect gate="1" pin="+" pad="6"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS1E-S-DC12V"/>
<attribute name="OC_FARNELL" value="1652598"/>
<attribute name="OC_NEWARK" value="13P3215"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS1E-S-DC24V"/>
<attribute name="OC_FARNELL" value="1372701"/>
<attribute name="OC_NEWARK" value="13P3216"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS1E-S-DC48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P3218"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1608323"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS1E-S-DC9V"/>
<attribute name="OC_FARNELL" value="1372683"/>
<attribute name="OC_NEWARK" value="13P3221"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS2E-L-*" prefix="K">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS &lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: &lt;a href="http://www.panasonic-electric-works.de/catalogues/downloads/relays/ds_61005_en_ds.pdf"&gt; Panasonic data sheet &lt;/a&gt;</description>
<gates>
<gate name="1" symbol="K+-R"/>
<gate name="2" symbol="K+-S"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="DS2E-L">
<connects>
<connect gate="1" pin="+" pad="2"/>
<connect gate="1" pin="-" pad="15"/>
<connect gate="2" pin="+" pad="1"/>
<connect gate="2" pin="-" pad="16"/>
<connect gate="3" pin="O" pad="6"/>
<connect gate="3" pin="P" pad="4"/>
<connect gate="3" pin="S" pad="8"/>
<connect gate="4" pin="O" pad="11"/>
<connect gate="4" pin="P" pad="13"/>
<connect gate="4" pin="S" pad="9"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="DS2E-SL-DC24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5812"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="DS2E-SL-DC5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5815"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS1E-L*" prefix="K">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS &lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
<gates>
<gate name="2" symbol="U"/>
<gate name="1" symbol="+KS+KR-"/>
</gates>
<devices>
<device name="" package="DS1E-L">
<connects>
<connect gate="1" pin="-" pad="3"/>
<connect gate="1" pin="R+" pad="6"/>
<connect gate="1" pin="S+" pad="1"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS1E-SL-DC12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P3222"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="DS1E-SL-DC48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5700"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="DS1E-SL-DC5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5701"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS4E-?*" prefix="K">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS &lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
<gate name="5" symbol="U"/>
</gates>
<devices>
<device name="" package="DS4E">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="16"/>
<connect gate="2" pin="O" pad="5"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="3" pin="O" pad="6"/>
<connect gate="3" pin="P" pad="4"/>
<connect gate="3" pin="S" pad="8"/>
<connect gate="4" pin="O" pad="11"/>
<connect gate="4" pin="P" pad="13"/>
<connect gate="4" pin="S" pad="9"/>
<connect gate="5" pin="O" pad="12"/>
<connect gate="5" pin="P" pad="14"/>
<connect gate="5" pin="S" pad="10"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L-" package="DS4E">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="16"/>
<connect gate="2" pin="O" pad="5"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="3" pin="O" pad="6"/>
<connect gate="3" pin="P" pad="4"/>
<connect gate="3" pin="S" pad="8"/>
<connect gate="4" pin="O" pad="11"/>
<connect gate="4" pin="P" pad="13"/>
<connect gate="4" pin="S" pad="9"/>
<connect gate="5" pin="O" pad="12"/>
<connect gate="5" pin="P" pad="14"/>
<connect gate="5" pin="S" pad="10"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS4E-L2-*" prefix="K">
<description>&lt;b&gt;DS-RELAYS HIGHLY SENSITIVE 1500 V FCC SURGE&lt;/b&gt; NAiS &lt;p&gt;
WITHSTANDING MINIATURE RELAY&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0001.pdf</description>
<gates>
<gate name="S" symbol="K+-"/>
<gate name="R" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="DS4E-L">
<connects>
<connect gate="1" pin="O" pad="5"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="7"/>
<connect gate="2" pin="O" pad="6"/>
<connect gate="2" pin="P" pad="4"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="O" pad="11"/>
<connect gate="3" pin="P" pad="13"/>
<connect gate="3" pin="S" pad="9"/>
<connect gate="4" pin="O" pad="12"/>
<connect gate="4" pin="P" pad="14"/>
<connect gate="4" pin="S" pad="10"/>
<connect gate="R" pin="+" pad="2"/>
<connect gate="R" pin="-" pad="15"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="16"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DSBT2-*" prefix="K">
<description>&lt;b&gt;DS-BT RELAYS 4,000 V BREAKDOWN VOLTAGE&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0010.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="DS-BT">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="16"/>
<connect gate="2" pin="O" pad="6"/>
<connect gate="2" pin="P" pad="4"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="O" pad="11"/>
<connect gate="3" pin="P" pad="13"/>
<connect gate="3" pin="S" pad="9"/>
</connects>
<technologies>
<technology name="M-2D-DC1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="M-2D-DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="M-2D-DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="M-2D-DC3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="M-2D-DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="M-2D-DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="M-2D-DC9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S-DC1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S-DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S-DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S-DC3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DSBT2-S-DC3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N4489"/>
</technology>
<technology name="S-DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S-DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S-DC9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS2Y-S-DC*" prefix="K">
<description>&lt;b&gt;MINIATURE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0023.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="DS2Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="16"/>
<connect gate="2" pin="O" pad="6"/>
<connect gate="2" pin="P" pad="4"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="O" pad="11"/>
<connect gate="3" pin="P" pad="13"/>
<connect gate="3" pin="S" pad="9"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-S-DC1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5827"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-S-DC12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P3261"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-S-DC24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P3264"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-S-DC3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5832"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-S-DC48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P3267"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-S-DC5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P3268"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-S-DC6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P3271"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-S-DC9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P3272"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DS2Y-SL2-DC*" prefix="K">
<description>&lt;b&gt;MINIATURE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61005_0023.pdf</description>
<gates>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
</gates>
<devices>
<device name="" package="DS2Y-2">
<connects>
<connect gate="1" pin="O" pad="6"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="8"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="13"/>
<connect gate="2" pin="S" pad="9"/>
<connect gate="R" pin="+" pad="2"/>
<connect gate="R" pin="-" pad="15"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="16"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-SL2-DC1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5841"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="DS2Y-SL2-DC12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="52F9208"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-SL2-DC24V"/>
<attribute name="OC_FARNELL" value="1372981"/>
<attribute name="OC_NEWARK" value="64K3125"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-SL2-DC3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="91B6712"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-SL2-DC48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5844"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="DS2Y-SL2-DC5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="93F4484"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-SL2-DC6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="99F8886"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="DS2Y-SL2-DC9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5848"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GN?*" prefix="K">
<description>&lt;b&gt;ULTRA-SMALL PACKAGE SLIM POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61007_0000.pdf</description>
<gates>
<gate name="R" symbol="K+-"/>
<gate name="S" symbol="U"/>
<gate name="T" symbol="U"/>
</gates>
<devices>
<device name="200" package="GN">
<connects>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="8"/>
<connect gate="S" pin="O" pad="2"/>
<connect gate="S" pin="P" pad="3"/>
<connect gate="S" pin="S" pad="4"/>
<connect gate="T" pin="O" pad="7"/>
<connect gate="T" pin="P" pad="6"/>
<connect gate="T" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN20003"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0830"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN20006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0831"/>
</technology>
<technology name="09">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGN20009"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3280"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN20012"/>
<attribute name="OC_FARNELL" value="3104783"/>
<attribute name="OC_NEWARK" value="13P0832"/>
</technology>
<technology name="1H">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGN2001H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3281"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN20024"/>
<attribute name="OC_FARNELL" value="4364211"/>
<attribute name="OC_NEWARK" value="13P0833"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN2004H"/>
<attribute name="OC_FARNELL" value="3104771"/>
<attribute name="OC_NEWARK" value="13P0834"/>
</technology>
</technologies>
</device>
<device name="210" package="GN">
<connects>
<connect gate="R" pin="+" pad="8"/>
<connect gate="R" pin="-" pad="1"/>
<connect gate="S" pin="O" pad="2"/>
<connect gate="S" pin="P" pad="3"/>
<connect gate="S" pin="S" pad="4"/>
<connect gate="T" pin="O" pad="7"/>
<connect gate="T" pin="P" pad="6"/>
<connect gate="T" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN21003"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8576"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN21006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8577"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN21012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8578"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN2104H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8579"/>
</technology>
</technologies>
</device>
<device name="200A" package="GN-A">
<connects>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="8"/>
<connect gate="S" pin="O" pad="2"/>
<connect gate="S" pin="P" pad="3"/>
<connect gate="S" pin="S" pad="4"/>
<connect gate="T" pin="O" pad="7"/>
<connect gate="T" pin="P" pad="6"/>
<connect gate="T" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200A03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0812"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200A06"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0814"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200A09Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0815"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200A12"/>
<attribute name="OC_FARNELL" value="3104801"/>
<attribute name="OC_NEWARK" value="13P0816"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200A24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0818"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200A4H"/>
<attribute name="OC_FARNELL" value="3104795"/>
<attribute name="OC_NEWARK" value="13P0820"/>
</technology>
</technologies>
</device>
<device name="200S" package="GN-S">
<connects>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="8"/>
<connect gate="S" pin="O" pad="2"/>
<connect gate="S" pin="P" pad="3"/>
<connect gate="S" pin="S" pad="4"/>
<connect gate="T" pin="O" pad="7"/>
<connect gate="T" pin="P" pad="6"/>
<connect gate="T" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200S03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0822"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200S12"/>
<attribute name="OC_FARNELL" value="1448335"/>
<attribute name="OC_NEWARK" value="13P0824"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value=""/>
<attribute name="OC_NEWARK" value=""/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200S24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0826"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN200S4H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0828"/>
</technology>
</technologies>
</device>
<device name="210A" package="GN-A">
<connects>
<connect gate="R" pin="+" pad="8"/>
<connect gate="R" pin="-" pad="1"/>
<connect gate="S" pin="O" pad="2"/>
<connect gate="S" pin="P" pad="3"/>
<connect gate="S" pin="S" pad="4"/>
<connect gate="T" pin="O" pad="7"/>
<connect gate="T" pin="P" pad="6"/>
<connect gate="T" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN210A03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8571"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGN210A12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3303"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN210A4H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8573"/>
</technology>
</technologies>
</device>
<device name="210S" package="GN-S">
<connects>
<connect gate="R" pin="+" pad="8"/>
<connect gate="R" pin="-" pad="1"/>
<connect gate="S" pin="O" pad="2"/>
<connect gate="S" pin="P" pad="3"/>
<connect gate="S" pin="S" pad="4"/>
<connect gate="T" pin="O" pad="7"/>
<connect gate="T" pin="P" pad="6"/>
<connect gate="T" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGN210S03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8575"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGN210S12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3320"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GQ?*" prefix="K">
<description>&lt;b&gt;ULTRA-SMALL PACKAGE FLAT POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61008_0000.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="200" package="GQ">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ20003"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0847"/>
</technology>
<technology name="06">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ20006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3360"/>
</technology>
<technology name="09">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ20009"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3361"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ20012"/>
<attribute name="OC_FARNELL" value="3104825"/>
<attribute name="OC_NEWARK" value="13P0849"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ20024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0850"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ2004H"/>
<attribute name="OC_FARNELL" value="3104813"/>
<attribute name="OC_NEWARK" value="13P0851"/>
</technology>
</technologies>
</device>
<device name="200A" package="GN-A">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ200A03"/>
<attribute name="OC_FARNELL" value="1448336"/>
<attribute name="OC_NEWARK" value="13P0835"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ200A09Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3339"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ200A12"/>
<attribute name="OC_FARNELL" value="3104849"/>
<attribute name="OC_NEWARK" value="13P0836"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ200A24"/>
<attribute name="OC_FARNELL" value="1448337"/>
<attribute name="OC_NEWARK" value="13P0837"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ200A4H"/>
<attribute name="OC_FARNELL" value="3104837"/>
<attribute name="OC_NEWARK" value="13P0838"/>
</technology>
</technologies>
</device>
<device name="200S" package="GN-S">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ200S03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3345"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ200S12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3353"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ200S1H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0842"/>
</technology>
<technology name="24">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ200S24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3355"/>
</technology>
<technology name="4H">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ200S4H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3357"/>
</technology>
</technologies>
</device>
<device name="210" package="GQ">
<connects>
<connect gate="1" pin="+" pad="8"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ21003"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3391"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ21009"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8586"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1H">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ2101H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3394"/>
</technology>
<technology name="24">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AGQ21024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C3396"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ2104H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8587"/>
</technology>
</technologies>
</device>
<device name="210A" package="GQ-A">
<connects>
<connect gate="1" pin="+" pad="8"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ210A03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8580"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ210A1H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8581"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ210A4H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8582"/>
</technology>
</technologies>
</device>
<device name="210S" package="GN-S">
<connects>
<connect gate="1" pin="+" pad="8"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AGQ210S4H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8583"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HX2-*" prefix="K">
<description>&lt;b&gt;Compact &amp; Slim 2 Form C Non-polarized Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61011_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="HX">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="12"/>
<connect gate="2" pin="O" pad="3"/>
<connect gate="2" pin="P" pad="4"/>
<connect gate="2" pin="S" pad="5"/>
<connect gate="3" pin="O" pad="10"/>
<connect gate="3" pin="P" pad="9"/>
<connect gate="3" pin="S" pad="8"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HY1*" prefix="K">
<description>&lt;b&gt;Non-polarized 1 Form C Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61012_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U1"/>
</gates>
<devices>
<device name="" package="HY">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="C@1"/>
<connect gate="2" pin="P@1" pad="C@2"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="-1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6688"/>
</technology>
<technology name="-24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6689"/>
</technology>
<technology name="-3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6690"/>
</technology>
<technology name="-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6692"/>
</technology>
<technology name="-6V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6693"/>
</technology>
<technology name="-9V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6694"/>
</technology>
<technology name="Z-1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Z-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1Z-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6704"/>
</technology>
<technology name="Z-24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1Z-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6705"/>
</technology>
<technology name="Z-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Z-4.5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1Z-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6707"/>
</technology>
<technology name="Z-5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1Z-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="52F9234"/>
</technology>
<technology name="Z-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="Z-9V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="HY1Z-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C6709"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="K2EBP*" prefix="K">
<description>&lt;b&gt;UNIQUELY DESIGNED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61013_0000.pdf</description>
<gates>
<gate name="_" symbol="K"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="K2EBP">
<connects>
<connect gate="1" pin="O" pad="NC1"/>
<connect gate="1" pin="P" pad="C1"/>
<connect gate="1" pin="S" pad="NO1"/>
<connect gate="2" pin="O" pad="NC2"/>
<connect gate="2" pin="P" pad="C2"/>
<connect gate="2" pin="S" pad="NO2"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="-110V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-12V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-28V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="K2-PS">
<connects>
<connect gate="1" pin="O" pad="NC1"/>
<connect gate="1" pin="P" pad="C1"/>
<connect gate="1" pin="S" pad="NO1"/>
<connect gate="2" pin="O" pad="NC2"/>
<connect gate="2" pin="P" pad="C2"/>
<connect gate="2" pin="S" pad="NO2"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="K4EBP*" prefix="K">
<description>&lt;b&gt;UNIQUELY DESIGNED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61013_0000.pdf</description>
<gates>
<gate name="_" symbol="K"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="K4EBP">
<connects>
<connect gate="1" pin="O" pad="NC1"/>
<connect gate="1" pin="P" pad="C1"/>
<connect gate="1" pin="S" pad="NO1"/>
<connect gate="2" pin="O" pad="NC2"/>
<connect gate="2" pin="P" pad="C2"/>
<connect gate="2" pin="S" pad="NO2"/>
<connect gate="3" pin="O" pad="NC3"/>
<connect gate="3" pin="P" pad="C3"/>
<connect gate="3" pin="S" pad="NO3"/>
<connect gate="4" pin="O" pad="NC4"/>
<connect gate="4" pin="P" pad="C4"/>
<connect gate="4" pin="S" pad="NO4"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="-110V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-12V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-28V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V-1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S" package="K4-PS">
<connects>
<connect gate="1" pin="O" pad="NC1"/>
<connect gate="1" pin="P" pad="C1"/>
<connect gate="1" pin="S" pad="NO1"/>
<connect gate="2" pin="O" pad="NC2"/>
<connect gate="2" pin="P" pad="C2"/>
<connect gate="2" pin="S" pad="NO2"/>
<connect gate="3" pin="O" pad="NC3"/>
<connect gate="3" pin="P" pad="C3"/>
<connect gate="3" pin="S" pad="NO3"/>
<connect gate="4" pin="O" pad="NC4"/>
<connect gate="4" pin="P" pad="C4"/>
<connect gate="4" pin="S" pad="NO4"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="K6EBP" prefix="K">
<description>&lt;b&gt;RELAY Socked&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61013_0000.pdf</description>
<gates>
<gate name="_" symbol="K"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
<gate name="5" symbol="U"/>
<gate name="6" symbol="U"/>
</gates>
<devices>
<device name="S" package="K6-PS">
<connects>
<connect gate="1" pin="O" pad="NC1"/>
<connect gate="1" pin="P" pad="C1"/>
<connect gate="1" pin="S" pad="NO1"/>
<connect gate="2" pin="O" pad="NC2"/>
<connect gate="2" pin="P" pad="C2"/>
<connect gate="2" pin="S" pad="NO2"/>
<connect gate="3" pin="O" pad="NC3"/>
<connect gate="3" pin="P" pad="C3"/>
<connect gate="3" pin="S" pad="NO3"/>
<connect gate="4" pin="O" pad="NC4"/>
<connect gate="4" pin="P" pad="C4"/>
<connect gate="4" pin="S" pad="NO4"/>
<connect gate="5" pin="O" pad="NC5"/>
<connect gate="5" pin="P" pad="C5"/>
<connect gate="5" pin="S" pad="NO5"/>
<connect gate="6" pin="O" pad="NC6"/>
<connect gate="6" pin="P" pad="C6"/>
<connect gate="6" pin="S" pad="NO6"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NF2EB-*" prefix="K">
<description>&lt;b&gt;FLATPACK RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61014_0000.pdf</description>
<gates>
<gate name="_" symbol="K"/>
<gate name="G$1" symbol="U"/>
<gate name="G$2" symbol="U"/>
</gates>
<devices>
<device name="" package="NF2">
<connects>
<connect gate="G$1" pin="O" pad="NC1"/>
<connect gate="G$1" pin="P" pad="C1"/>
<connect gate="G$1" pin="S" pad="NO1"/>
<connect gate="G$2" pin="O" pad="NC2"/>
<connect gate="G$2" pin="P" pad="C2"/>
<connect gate="G$2" pin="S" pad="NO2"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NF2EB-12V"/>
<attribute name="OC_FARNELL" value="1200946"/>
<attribute name="OC_NEWARK" value="13P5536"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NF2EB-24V"/>
<attribute name="OC_FARNELL" value="1175714"/>
<attribute name="OC_NEWARK" value="13P5537"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NF2EB-5V"/>
<attribute name="OC_FARNELL" value="1703747"/>
<attribute name="OC_NEWARK" value="13P5538"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NF2EB-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P5539"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NF4EB-*" prefix="K">
<description>&lt;b&gt;FLATPACK RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61014_0000.pdf</description>
<gates>
<gate name="_" symbol="K"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="NF4">
<connects>
<connect gate="1" pin="O" pad="NC1"/>
<connect gate="1" pin="P" pad="C1"/>
<connect gate="1" pin="S" pad="NO1"/>
<connect gate="2" pin="O" pad="NC2"/>
<connect gate="2" pin="P" pad="C2"/>
<connect gate="2" pin="S" pad="NO2"/>
<connect gate="3" pin="O" pad="NC3"/>
<connect gate="3" pin="P" pad="C3"/>
<connect gate="3" pin="S" pad="NO3"/>
<connect gate="4" pin="O" pad="NC4"/>
<connect gate="4" pin="P" pad="C4"/>
<connect gate="4" pin="S" pad="NO4"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NF4EB-12V"/>
<attribute name="OC_FARNELL" value="1175715"/>
<attribute name="OC_NEWARK" value="13P5540"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NF4EB-24V"/>
<attribute name="OC_FARNELL" value="1373470"/>
<attribute name="OC_NEWARK" value="13P5541"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NF4EB-48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P5542"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="NF4EB-5V"/>
<attribute name="OC_FARNELL" value="1200947"/>
<attribute name="OC_NEWARK" value="13P5543"/>
</technology>
<technology name="6V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="NF4EB-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="46F5739"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL6EBX-*" prefix="K">
<description>&lt;b&gt;6PDT FLATPACK 2AMP DIL RELAY&lt;/b&gt; NAiS&lt;p&gt;
Single side stable&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61014_0003.pdf</description>
<gates>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
<gate name="5" symbol="U"/>
<gate name="6" symbol="U"/>
<gate name="-" symbol="K+-"/>
</gates>
<devices>
<device name="" package="NL6EBX">
<connects>
<connect gate="-" pin="+" pad="5"/>
<connect gate="-" pin="-" pad="6"/>
<connect gate="1" pin="O" pad="21"/>
<connect gate="1" pin="P" pad="1"/>
<connect gate="1" pin="S" pad="22"/>
<connect gate="2" pin="O" pad="20"/>
<connect gate="2" pin="P" pad="2"/>
<connect gate="2" pin="S" pad="18"/>
<connect gate="3" pin="O" pad="19"/>
<connect gate="3" pin="P" pad="3"/>
<connect gate="3" pin="S" pad="17"/>
<connect gate="4" pin="O" pad="14"/>
<connect gate="4" pin="P" pad="8"/>
<connect gate="4" pin="S" pad="16"/>
<connect gate="5" pin="O" pad="13"/>
<connect gate="5" pin="P" pad="9"/>
<connect gate="5" pin="S" pad="15"/>
<connect gate="6" pin="O" pad="12"/>
<connect gate="6" pin="P" pad="10"/>
<connect gate="6" pin="S" pad="11"/>
</connects>
<technologies>
<technology name="DC110V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC60V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NL6EBX-L2-*" prefix="K">
<description>&lt;b&gt;6PDT FLATPACK 2AMP DIL RELAY&lt;/b&gt; NAiS&lt;p&gt;
2 coil latching&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61014_0003.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
<gate name="5" symbol="U"/>
<gate name="6" symbol="U"/>
</gates>
<devices>
<device name="" package="NL6EBX-L2">
<connects>
<connect gate="1" pin="O" pad="21"/>
<connect gate="1" pin="P" pad="1"/>
<connect gate="1" pin="S" pad="22"/>
<connect gate="2" pin="O" pad="20"/>
<connect gate="2" pin="P" pad="2"/>
<connect gate="2" pin="S" pad="18"/>
<connect gate="3" pin="O" pad="19"/>
<connect gate="3" pin="P" pad="3"/>
<connect gate="3" pin="S" pad="17"/>
<connect gate="4" pin="O" pad="14"/>
<connect gate="4" pin="P" pad="8"/>
<connect gate="4" pin="S" pad="16"/>
<connect gate="5" pin="O" pad="13"/>
<connect gate="5" pin="P" pad="9"/>
<connect gate="5" pin="S" pad="15"/>
<connect gate="6" pin="O" pad="12"/>
<connect gate="6" pin="P" pad="10"/>
<connect gate="6" pin="S" pad="11"/>
<connect gate="R" pin="+" pad="4"/>
<connect gate="R" pin="-" pad="7"/>
<connect gate="S" pin="+" pad="5"/>
<connect gate="S" pin="-" pad="6"/>
</connects>
<technologies>
<technology name="DC110V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC60V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TF2-?*" prefix="K">
<description>&lt;b&gt;SMALL POLARIZED RELAY WITH HIGH SENSITIVITY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61017_0000.pdf</description>
<gates>
<gate name="-" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="TF2">
<connects>
<connect gate="-" pin="+" pad="1"/>
<connect gate="-" pin="-" pad="10"/>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L" package="TF2">
<connects>
<connect gate="-" pin="+" pad="10"/>
<connect gate="-" pin="-" pad="1"/>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="846004"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TF2-L2*" prefix="K">
<description>&lt;b&gt;SMALL POLARIZED RELAY WITH HIGH SENSITIVITY&lt;/b&gt; NAiS&lt;p&gt;
2 coil latching&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61017_0000.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="TF2">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="R" pin="+" pad="10"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="5"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TK1-?*" prefix="K">
<description>&lt;b&gt;ULTRA LOW PROFILE 2 AMP. POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61018_0000.pdf</description>
<gates>
<gate name="-" symbol="K+-"/>
<gate name="1" symbol="U"/>
</gates>
<devices>
<device name="" package="TK">
<connects>
<connect gate="-" pin="+" pad="1"/>
<connect gate="-" pin="-" pad="3"/>
<connect gate="1" pin="O" pad="4"/>
<connect gate="1" pin="P" pad="5"/>
<connect gate="1" pin="S" pad="6"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TK1-12V"/>
<attribute name="OC_FARNELL" value="1380961"/>
<attribute name="OC_NEWARK" value="67K1254"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TK1-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="64K3182"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9053"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9054"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TK1-5V"/>
<attribute name="OC_FARNELL" value="1380960"/>
<attribute name="OC_NEWARK" value="64K3183"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9056"/>
</technology>
<technology name="9V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TK1-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9734"/>
</technology>
<technology name="H-1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L-" package="TK">
<connects>
<connect gate="-" pin="+" pad="3"/>
<connect gate="-" pin="-" pad="1"/>
<connect gate="1" pin="O" pad="4"/>
<connect gate="1" pin="P" pad="5"/>
<connect gate="1" pin="S" pad="6"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TK1-L-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9715"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9750"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TK1-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9718"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TK1-L-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9720"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-L-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9050"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TK1-L2-*" prefix="K">
<description>&lt;b&gt;ULTRA LOW PROFILE 2 AMP. POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
2 coil latching&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61018_0000.pdf</description>
<gates>
<gate name="-" symbol="+KS+KR-"/>
<gate name="G$1" symbol="U"/>
</gates>
<devices>
<device name="" package="TK">
<connects>
<connect gate="-" pin="-" pad="2"/>
<connect gate="-" pin="R+" pad="1"/>
<connect gate="-" pin="S+" pad="3"/>
<connect gate="G$1" pin="O" pad="4"/>
<connect gate="G$1" pin="P" pad="5"/>
<connect gate="G$1" pin="S" pad="6"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-L2-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9751"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-L2-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9752"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-L2-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9753"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-L2-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9754"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TK1-L2-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9755"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TN2?-*" prefix="K">
<description>&lt;b&gt;SLIM POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61019_0000.pdf</description>
<gates>
<gate name="-" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="TN2">
<connects>
<connect gate="-" pin="+" pad="1"/>
<connect gate="-" pin="-" pad="10"/>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-12V"/>
<attribute name="OC_FARNELL" value="1200956"/>
<attribute name="OC_NEWARK" value="65K1079"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-24V"/>
<attribute name="OC_FARNELL" value="910405"/>
<attribute name="OC_NEWARK" value="64K3187"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90F3177"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-4.5V"/>
<attribute name="OC_FARNELL" value="1231845"/>
<attribute name="OC_NEWARK" value="64K3188"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TN2-48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9184"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-5V"/>
<attribute name="OC_FARNELL" value="1200955"/>
<attribute name="OC_NEWARK" value="64K3189"/>
</technology>
<technology name="6V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90F3180"/>
</technology>
<technology name="9V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90F3181"/>
</technology>
</technologies>
</device>
<device name="-L" package="TN2">
<connects>
<connect gate="-" pin="+" pad="10"/>
<connect gate="-" pin="-" pad="1"/>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90F3171"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90F3184"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TN2-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9757"/>
</technology>
<technology name="5.">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TN2-L-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90F3169"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TN-L2-*" prefix="K">
<description>&lt;b&gt;SLIM POLARIZED RELAY&lt;/b&gt; NAiS&lt;p&gt;
2 coil latched&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61019_0000.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="TN2">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="R" pin="+" pad="10"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="5"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TQ2?*" prefix="K">
<description>&lt;b&gt;LOW PROFILE 2 FORM C RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61020_0001.pdf
Source: http://www.mew-europe.com/..  en_ds_61020_0004.pdf</description>
<gates>
<gate name="_" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="-" package="TQ2">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="10"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-12V"/>
<attribute name="OC_FARNELL" value="1200949"/>
<attribute name="OC_NEWARK" value="64K3197"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-24V"/>
<attribute name="OC_FARNELL" value="1175717"/>
<attribute name="OC_NEWARK" value="64K3198"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-3V"/>
<attribute name="OC_FARNELL" value="1703746"/>
<attribute name="OC_NEWARK" value="73K2455"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-4.5V"/>
<attribute name="OC_FARNELL" value="1163566"/>
<attribute name="OC_NEWARK" value="64K3199"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2-48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9197"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-5V"/>
<attribute name="OC_FARNELL" value="1175716"/>
<attribute name="OC_NEWARK" value="64K3200"/>
</technology>
<technology name="6V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="64K3201"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9201"/>
</technology>
</technologies>
</device>
<device name="-L-" package="TQ2">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="_" pin="+" pad="10"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="64K3190"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="87F3168"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9767"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-L-5V"/>
<attribute name="OC_FARNELL" value="1448361"/>
<attribute name="OC_NEWARK" value="64K3191"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-SA-" package="TQ-SA">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="10"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-1.5V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9205"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SA-12V"/>
<attribute name="OC_FARNELL" value="1124056"/>
<attribute name="OC_NEWARK" value="64K3203"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9208"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9847"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92B3979"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9215"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SA-5V"/>
<attribute name="OC_FARNELL" value="1124054"/>
<attribute name="OC_NEWARK" value="64K3205"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9219"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9220"/>
</technology>
</technologies>
</device>
<device name="SA-L-" package="TQ-SA">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="_" pin="+" pad="10"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9777"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9778"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9779"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-L-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9780"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-SL-" package="TQ-SL">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="10"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SL-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9222"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SL-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9224"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SL-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9226"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SL-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9228"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SL-L-" package="TQ-SL">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="_" pin="+" pad="10"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SL-L-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9870"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SL-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9793"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-SS-" package="TQ-SS">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="10"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9230"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9231"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-24V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9232"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SS-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9995"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9234"/>
</technology>
<technology name="48V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SS-48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0002"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SS-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0005"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SS-L-" package="TQ-SS">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="_" pin="+" pad="10"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SS-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9950"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-L-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9797"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TQ2?-L2-*" prefix="K">
<description>&lt;b&gt;LOW PROFILE 2 FORM C RELAY&lt;/b&gt; NAiS&lt;p&gt;
2 coil latching&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61020_0001.pdf
Source: http://www.mew-europe.com/..  en_ds_61020_0002.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="TQ2">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="R" pin="+" pad="10"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2-L2-9V"/>
<attribute name="OC_FARNELL" value="1217662"/>
<attribute name="OC_NEWARK" value="64K3196"/>
</technology>
</technologies>
</device>
<device name="SA" package="TQ-SA">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="R" pin="+" pad="10"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="5"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-L2-12V"/>
<attribute name="OC_FARNELL" value="1124058"/>
<attribute name="OC_NEWARK" value="02M6304"/>
</technology>
<technology name="24V">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="TQ2SA-L2-24V"/>
<attribute name="OC_FARNELL" value="625784"/>
<attribute name="OC_NEWARK" value="15J0011"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-L2-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9786"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SA-L2-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9788"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SA-L2-5V"/>
<attribute name="OC_FARNELL" value="625760"/>
<attribute name="OC_NEWARK" value="64K3202"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SL" package="TQ-SL">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="R" pin="+" pad="10"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="5"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SL-L2-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9794"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SL-L2-3V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9899"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SL-L2-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9795"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SL-L2-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9796"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SS" package="TQ-SS">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="R" pin="+" pad="10"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="5"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-L2-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9800"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-L2-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9801"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-L2-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9802"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ2SS-L2-4.5V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9803"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ2SS-L2-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="64K3206"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TQ4-L2-*" prefix="K">
<description>&lt;b&gt;LOW PROFILE 2 FORM C RELAY&lt;/b&gt; NAiS&lt;p&gt;
2 coil latching&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61020_0001.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="TQ4">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="6"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="O" pad="18"/>
<connect gate="3" pin="P" pad="17"/>
<connect gate="3" pin="S" pad="16"/>
<connect gate="4" pin="O" pad="15"/>
<connect gate="4" pin="P" pad="14"/>
<connect gate="4" pin="S" pad="13"/>
<connect gate="R" pin="+" pad="20"/>
<connect gate="R" pin="-" pad="11"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="10"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ4-L2-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="90F5822"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ4-L2-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9807"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ4-L2-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="64K3208"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TQ4-*" prefix="K">
<description>&lt;b&gt;LOW PROFILE 2 FORM C RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61020_0001.pdf</description>
<gates>
<gate name="_" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="TQ4">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="6"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="O" pad="18"/>
<connect gate="3" pin="P" pad="17"/>
<connect gate="3" pin="S" pad="16"/>
<connect gate="4" pin="O" pad="15"/>
<connect gate="4" pin="P" pad="14"/>
<connect gate="4" pin="S" pad="13"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="10"/>
</connects>
<technologies>
<technology name="12C">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ4-24V"/>
<attribute name="OC_FARNELL" value="1608334"/>
<attribute name="OC_NEWARK" value="64K3210"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ4-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9240"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TQ4-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9241"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TQ4-5V"/>
<attribute name="OC_FARNELL" value="1448362"/>
<attribute name="OC_NEWARK" value="67K1293"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="L-" package="TQ4">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="6"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="O" pad="18"/>
<connect gate="3" pin="P" pad="17"/>
<connect gate="3" pin="S" pad="16"/>
<connect gate="4" pin="O" pad="15"/>
<connect gate="4" pin="P" pad="14"/>
<connect gate="4" pin="S" pad="13"/>
<connect gate="_" pin="+" pad="10"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1448362"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TX2?-*" prefix="K">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
<gates>
<gate name="_" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="TX2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9570"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2-12V"/>
<attribute name="OC_FARNELL" value="1200952"/>
<attribute name="OC_NEWARK" value="67K1295"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2-24V"/>
<attribute name="OC_FARNELL" value="1124059"/>
<attribute name="OC_NEWARK" value="64K3215"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9573"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2-4.5V"/>
<attribute name="OC_FARNELL" value="1200950"/>
<attribute name="OC_NEWARK" value="64K3216"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2-5V"/>
<attribute name="OC_FARNELL" value="1200950"/>
<attribute name="OC_NEWARK" value="67K1296"/>
</technology>
<technology name="6V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0387"/>
</technology>
<technology name="9V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0388"/>
</technology>
</technologies>
</device>
<device name="SA" package="TX2SA">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2SA-12V"/>
<attribute name="OC_FARNELL" value="910480"/>
<attribute name="OC_NEWARK" value="64K3217"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2SA-24V"/>
<attribute name="OC_FARNELL" value="1652603"/>
<attribute name="OC_NEWARK" value="64K3218"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9584"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2SA-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92F1604"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-5V"/>
<attribute name="OC_FARNELL" value="1200957"/>
<attribute name="OC_NEWARK" value="13P9589"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-6V-X"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9592"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9593"/>
</technology>
</technologies>
</device>
<device name="-L" package="TX2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0367"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L-24V-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3976"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9975"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9976"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9977"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9978"/>
</technology>
</technologies>
</device>
<device name="SL" package="TX2SL">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2SL-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0519"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16P9442"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9598"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9600"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9602"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9603"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-9V-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6123"/>
</technology>
</technologies>
</device>
<device name="SS" package="TX2SS">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SS-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9605"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SS-3V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9606"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SS-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9607"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SS-48V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9609"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SS-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9610"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SA-L" package="TX2SA">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SL-L" package="TX2SL">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-L-24V-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3990"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2SL-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0477"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SS-L" package="TX2SS">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2SS-L-12V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0549"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SS-L-3V-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3991"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TX2?-L2-*" prefix="K">
<description>&lt;b&gt;TX Relay 2 coil latching&lt;/b&gt; NAiS&lt;p&gt;
&lt;hr&gt;
2 AMP. HIGH CAPACITY RELAY WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf
&lt;hr&gt;
TX-S
SMALL POLARIZED WITH HIGH SENSITIVITY 50mW
Source: http://www.mew-europe.com/..  en_ds_61022_0022.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="TX2-L2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="12"/>
<connect gate="S" pin="-" pad="7"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2-L2-12V"/>
<attribute name="OC_FARNELL" value="1124060"/>
<attribute name="OC_NEWARK" value="64K3213"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L2-24V"/>
<attribute name="OC_FARNELL" value="1124061"/>
<attribute name="OC_NEWARK" value="31M0467"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L2-3V-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3980"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L2-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9981"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L2-5V"/>
<attribute name="OC_FARNELL" value="625826"/>
<attribute name="OC_NEWARK" value="15P9982"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2-L2-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9984"/>
</technology>
</technologies>
</device>
<device name="SA" package="TX2SA-L2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="12"/>
<connect gate="S" pin="-" pad="7"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TX2SA-L2-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92F1610"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-L2-24V-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3986"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-L2-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9991"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-L2-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9993"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-L2-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9995"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SA-L2-6V-X"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9578"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SL" package="TX2SL-L2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="12"/>
<connect gate="S" pin="-" pad="7"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-L2-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9998"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-L2-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16P0001"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SL-L2-9V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16P0002"/>
</technology>
</technologies>
</device>
<device name="SS" package="TX2SS-L2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="12"/>
<connect gate="S" pin="-" pad="7"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TX2SS-L2-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16P0003"/>
</technology>
</technologies>
</device>
<device name="S2SA" package="TX2SA-L2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="12"/>
<connect gate="S" pin="-" pad="7"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S2SL" package="TX2SL-L2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="12"/>
<connect gate="S" pin="-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S2SS" package="TX2SS-L2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="12"/>
<connect gate="S" pin="-" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TX?-*" prefix="K">
<description>&lt;b&gt;TX Relais&lt;/b&gt; NAiS&lt;p&gt;
&lt;hr&gt;
TX-D RELAYS HIGH INSULATION&lt;br&gt;
Conforming to the supplementary insulation class of EN Standards (EN41003)&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0007.pdf
&lt;hr&gt;
TX-S RELAYS SMALL POLARIZED RELAY WITH HIGH SENSITIVITY 50mW&lt;br&gt;
Source: http://www.mew-europe.com/..  en_ds_61022_0022.pdf</description>
<gates>
<gate name="_" symbol="K+-"/>
<gate name="G$1" symbol="U"/>
<gate name="G$2" symbol="U"/>
</gates>
<devices>
<device name="D2" package="TXD2">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9522"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9523"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9524"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9525"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SA" package="TXD2SA">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SA-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9526"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TXD2SA-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0176"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SA-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9531"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SA-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9532"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SA-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9534"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SL" package="TXD2SL">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TXD2SL-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0248"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SL-4.5V-X"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6056"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SS" package="TXD2SS">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SS-12V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9535"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SS-24V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9536"/>
</technology>
<technology name="3V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TXD2SS-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0320"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TXD2SS-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0326"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2-L" package="TXD2">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TXD2-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0103"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SA-L" package="TXD2SA">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SL-L" package="TXD2SL">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SL-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9956"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SL-L-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9958"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXD2SL-L-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9960"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SS-L" package="TXD2SS">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2-2M" package="TXD2">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SA-2M" package="TXD2SA">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SL-2M" package="TXD2SL">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="D2SS-2M" package="TXD2SS">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TXD2SS-2M-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0296"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="S2" package="TXD2">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9539"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9540"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9541"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-4.5V"/>
<attribute name="OC_FARNELL" value="1608335"/>
<attribute name="OC_NEWARK" value="13P9542"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9543"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6058"/>
</technology>
</technologies>
</device>
<device name="S2-L" package="TXD2">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-L-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3844"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3845"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-L-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3846"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9962"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9963"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2-L-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3848"/>
</technology>
</technologies>
</device>
<device name="S2SA-" package="TXD2SA">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6059"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-12V"/>
<attribute name="OC_FARNELL" value="1231846"/>
<attribute name="OC_NEWARK" value="13P9545"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TXS2SA-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11C0345"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6066"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9550"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9552"/>
</technology>
<technology name="9V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="TXS2SA-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="97H8371"/>
</technology>
</technologies>
</device>
<device name="S2SL-" package="TXD2SL">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6074"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6077"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6081"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-3V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9555"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9556"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6087"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6090"/>
</technology>
</technologies>
</device>
<device name="S2SS-" package="TXD2SS">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6094"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9561"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-24V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9563"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-3V-Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9564"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P9565"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6103"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N6106"/>
</technology>
</technologies>
</device>
<device name="S2SA-L-" package="TXD2SA">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-L-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3853"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3856"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-L-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3859"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3862"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P9968"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-L-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3867"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-L-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3870"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SA-L-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3873"/>
</technology>
</technologies>
</device>
<device name="S2SL-L" package="TXD2SL">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-L-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3892"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3895"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-L-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3898"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3902"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3905"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-L-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3908"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SL-L-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3911"/>
</technology>
</technologies>
</device>
<device name="S2SS-L" package="TXD2SS">
<connects>
<connect gate="G$1" pin="O" pad="3"/>
<connect gate="G$1" pin="P" pad="4"/>
<connect gate="G$1" pin="S" pad="5"/>
<connect gate="G$2" pin="O" pad="10"/>
<connect gate="G$2" pin="P" pad="9"/>
<connect gate="G$2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-L-1.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3933"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-L-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3936"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-L-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3939"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-L-3V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3942"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3945"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-L-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3948"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="TXS2SS-L-9V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3951"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TX2SO?-*" prefix="K">
<description>&lt;b&gt;2 AMP. HIGH CAPACITY RELAY&lt;/b&gt; NAiS&lt;p&gt;WITH HIGH SURGE VOLTAGE &amp; HIGH BREAKDOWN VOLTAGE&lt;br&gt;Source: http://www.mew-europe.com/..  en_ds_61022_0001.pdf</description>
<gates>
<gate name="_" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="TX2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SA" package="TX2SA">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-L" package="TX2">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SL" package="TX2SL">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SS" package="TX2SS">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="1"/>
<connect gate="_" pin="-" pad="12"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SA-L" package="TX2SA">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SL-L" package="TX2SL">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="SS-L" package="TX2SS">
<connects>
<connect gate="1" pin="O" pad="3"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="5"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="9"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="_" pin="+" pad="12"/>
<connect gate="_" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD?*" prefix="K">
<description>&lt;b&gt;Slim Power Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61112_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="1" package="LD">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="3727154"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="ALD112"/>
<attribute name="OC_FARNELL" value="3727166"/>
<attribute name="OC_NEWARK" value="70C6003"/>
</technology>
<technology name="18">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="3727178"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PE10?*" prefix="K">
<description>&lt;b&gt;SLIM POWER Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61122_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="PE-FORM-A">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2525"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2526"/>
</technology>
<technology name="018">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10018"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2527"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2528"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="27M3556"/>
</technology>
<technology name="04H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE1004H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2529"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10060"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2530"/>
</technology>
<technology name="105">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="106">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10106"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2531"/>
</technology>
<technology name="112">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10112"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2532"/>
</technology>
<technology name="118">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10118"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2533"/>
</technology>
<technology name="124">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10124"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2534"/>
</technology>
<technology name="148">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10148"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2536"/>
</technology>
<technology name="14H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE1014H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2535"/>
</technology>
<technology name="160">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE10160"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2537"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PE30?*" prefix="K">
<description>&lt;b&gt;SLIM POWER Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61122_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="PE-FORM-C">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE30006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2538"/>
</technology>
<technology name="012">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="APE30012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="37J1097"/>
</technology>
<technology name="018">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE30018"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2539"/>
</technology>
<technology name="024">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="APE30024"/>
<attribute name="OC_FARNELL" value="1703738"/>
<attribute name="OC_NEWARK" value="01H7899"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE30048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2540"/>
</technology>
<technology name="04H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE3004H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="55M0343"/>
</technology>
<technology name="060">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="APE30060"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13J1294"/>
</technology>
<technology name="105">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="106">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="112">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE30112"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0932"/>
</technology>
<technology name="118">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE30118"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2542"/>
</technology>
<technology name="124">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE30124"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P0933"/>
</technology>
<technology name="148">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE30148"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2543"/>
</technology>
<technology name="14H">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="APE3014H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="36K1690"/>
</technology>
<technology name="160">
<attribute name="MF" value=""/>
<attribute name="MPN" value="APE30160"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2544"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PE-PS" prefix="K">
<description>&lt;b&gt;SLIM POWER Relay SOCKET&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61122_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="-LED" symbol="LED"/>
</gates>
<devices>
<device name="" package="PE-SOCKET">
<connects>
<connect gate="-LED" pin="A" pad="+LED"/>
<connect gate="-LED" pin="C" pad="-LED"/>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PA?*" prefix="K">
<description>&lt;b&gt;SLIM POWER RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61123_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="1A-" package="PA">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="PA1A-12V-Y1"/>
<attribute name="OC_FARNELL" value="910363"/>
<attribute name="OC_NEWARK" value="82H8374"/>
</technology>
<technology name="18V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="PA1A-18V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92B3524"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PA1A-24V"/>
<attribute name="OC_FARNELL" value="910375"/>
<attribute name="OC_NEWARK" value="13P6167"/>
</technology>
<technology name="6VV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9VV">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="1A-SOCKED-S" package="PA-STD-SOCKET">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="1A-SOCKED-C" package="PA-CLI-SOCKET">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CB*" prefix="K">
<description>&lt;b&gt;HIGH POWER AUTOMOTIVE RELAY Form A&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61202_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="CB1">
<connects>
<connect gate="1" pin="1" pad="86"/>
<connect gate="1" pin="2" pad="85"/>
<connect gate="2" pin="P" pad="30"/>
<connect gate="2" pin="S" pad="87"/>
</connects>
<technologies>
<technology name="1A-P-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CB1A-P-12V"/>
<attribute name="OC_FARNELL" value="1270582"/>
<attribute name="OC_NEWARK" value="50B849"/>
</technology>
<technology name="1A-P-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CB1A-P-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P2833"/>
</technology>
<technology name="1A-T-P-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CB1A-T-P-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="26H6273"/>
</technology>
<technology name="1A-T-P-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CB1*" prefix="K">
<description>&lt;b&gt;HIGH POWER AUTOMOTIVE RELAY Form C&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61202_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="CB1">
<connects>
<connect gate="1" pin="1" pad="86"/>
<connect gate="1" pin="2" pad="85"/>
<connect gate="2" pin="O" pad="87A"/>
<connect gate="2" pin="P" pad="30"/>
<connect gate="2" pin="S" pad="87"/>
</connects>
<technologies>
<technology name="-P-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CB1-P-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="52F9201"/>
</technology>
<technology name="-P-24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CB1-P-24V"/>
<attribute name="OC_FARNELL" value="4168987"/>
<attribute name="OC_NEWARK" value="07C0827"/>
</technology>
<technology name="F-P-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CB1F-P-12V"/>
<attribute name="OC_FARNELL" value="1414069"/>
<attribute name="OC_NEWARK" value="50F4024"/>
</technology>
<technology name="F-P-24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CB1F-P-24V"/>
<attribute name="OC_FARNELL" value="1423191"/>
<attribute name="OC_NEWARK" value="94B6706"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CB1*V" prefix="K">
<description>&lt;b&gt;HIGH POWER AUTOMOTIVE RELAY Form A with Diode&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61202_0000.pdf</description>
<gates>
<gate name="1" symbol="K+-D"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="CB1">
<connects>
<connect gate="1" pin="+" pad="86"/>
<connect gate="1" pin="-" pad="85"/>
<connect gate="2" pin="P" pad="30"/>
<connect gate="2" pin="S" pad="87"/>
</connects>
<technologies>
<technology name="-D-P-12">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CB1-D-P-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5390"/>
</technology>
<technology name="-D-P-24">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CB1-D-P-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5392"/>
</technology>
<technology name="A-D-P-12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CB1A-D-P-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P2827"/>
</technology>
<technology name="A-D-P-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A-T-D-P-12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A-T-D-P-24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CF2*" prefix="K">
<description>&lt;b&gt;NEW DUAL POWER AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61203_0000.pdf</description>
<gates>
<gate name="1-1" symbol="K"/>
<gate name="1-2" symbol="K"/>
<gate name="2" symbol="CF"/>
</gates>
<devices>
<device name="" package="CF">
<connects>
<connect gate="1-1" pin="1" pad="1"/>
<connect gate="1-1" pin="2" pad="1A"/>
<connect gate="1-2" pin="1" pad="2"/>
<connect gate="1-2" pin="2" pad="2A"/>
<connect gate="2" pin="COM1" pad="C1"/>
<connect gate="2" pin="COM2" pad="C2"/>
<connect gate="2" pin="NC" pad="NC"/>
<connect gate="2" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CM1A*" prefix="K">
<description>&lt;b&gt;AUTOMOTIVE MICRO-ISO RELAY&lt;/b&gt; NAiS&lt;p&gt;
en_ds_61204_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="CM">
<connects>
<connect gate="1" pin="1" pad="85"/>
<connect gate="1" pin="2" pad="86"/>
<connect gate="2" pin="P" pad="30"/>
<connect gate="2" pin="S" pad="87"/>
</connects>
<technologies>
<technology name="-P-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CM1A-P-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5491"/>
</technology>
<technology name="-P-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-P-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CM1AF-P-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5497"/>
</technology>
<technology name="F-P-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CM1*" prefix="K">
<description>&lt;b&gt;AUTOMOTIVE MICRO-ISO RELAY&lt;/b&gt; NAiS&lt;p&gt;
en_ds_61204_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="CM">
<connects>
<connect gate="1" pin="1" pad="85"/>
<connect gate="1" pin="2" pad="86"/>
<connect gate="2" pin="O" pad="87A"/>
<connect gate="2" pin="P" pad="30"/>
<connect gate="2" pin="S" pad="87"/>
</connects>
<technologies>
<technology name="-P-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CM1-P-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="50B850"/>
</technology>
<technology name="-P-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-P-12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CM1F-P-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5503"/>
</technology>
<technology name="F-P-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CT112" prefix="K">
<description>&lt;b&gt;ULTRA SMALL AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Slim 1c type &lt;br&gt;
en_ds_61205_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="CT-SLIM">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CT512" prefix="K">
<description>&lt;b&gt;ULTRA SMALL AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Twin type (10 terminals)&lt;br&gt;
en_ds_61205_0000.pdf</description>
<gates>
<gate name="A" symbol="K"/>
<gate name="B" symbol="K"/>
<gate name="A1" symbol="U"/>
<gate name="B1" symbol="U"/>
</gates>
<devices>
<device name="" package="CT2-TWIN">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="1A"/>
<connect gate="A1" pin="O" pad="NC1"/>
<connect gate="A1" pin="P" pad="C1"/>
<connect gate="A1" pin="S" pad="NO1"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="2A"/>
<connect gate="B1" pin="O" pad="NC2"/>
<connect gate="B1" pin="P" pad="C2"/>
<connect gate="B1" pin="S" pad="NO2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CT212" prefix="K">
<description>&lt;b&gt;ULTRA SMALL AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Twin type (8 terminals)&lt;br&gt;
en_ds_61205_0000.pdf</description>
<gates>
<gate name="A" symbol="K"/>
<gate name="B" symbol="K"/>
<gate name="1" symbol="CF"/>
</gates>
<devices>
<device name="" package="CT-TWIN">
<connects>
<connect gate="1" pin="COM1" pad="C1"/>
<connect gate="1" pin="COM2" pad="C2"/>
<connect gate="1" pin="NC" pad="NC"/>
<connect gate="1" pin="NO" pad="NO"/>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="1A"/>
<connect gate="B" pin="1" pad="2"/>
<connect gate="B" pin="2" pad="2A"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP1A" prefix="K">
<description>&lt;b&gt;ULTRA-MINIATURE LOW PROFILE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61207_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="CP1A">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CP1A-12V"/>
<attribute name="OC_FARNELL" value="1629083"/>
<attribute name="OC_NEWARK" value="10C5509"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CP1?-*" prefix="K">
<description>&lt;b&gt;ULTRA-MINIATURE LOW PROFILE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61207_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="CP1">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CP1-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5508"/>
</technology>
</technologies>
</device>
<device name="SA" package="CP1SA">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="CP1SA-12V-X"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96K2384"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CQ1-12V" prefix="K">
<description>&lt;b&gt;AUTOMOTIVE QUIET RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61208_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="CQ1">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CR2-12V" prefix="KI">
<description>&lt;b&gt;DUAL POWER QUIET AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61209_0000.pdf</description>
<gates>
<gate name="1" symbol="K2-1"/>
<gate name="2" symbol="CF"/>
</gates>
<devices>
<device name="" package="CR2">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="1" pin="M" pad="M"/>
<connect gate="2" pin="COM1" pad="C1"/>
<connect gate="2" pin="COM2" pad="C2"/>
<connect gate="2" pin="NC" pad="NC"/>
<connect gate="2" pin="NO" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="CR2-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C5511"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JJM1A-12V" prefix="K">
<description>&lt;b&gt;HALF-SIZE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61210_0001.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="JJM1A">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JJM1-12V" prefix="K">
<description>&lt;b&gt;HALF-SIZE AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61210_0001.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="JJM1C">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="JJM1-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C7318"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JJM2W-12V" prefix="K">
<description>&lt;b&gt;DOUBLE MAKE CONTACT AUTOMOTIVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61210_0002.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S2"/>
</gates>
<devices>
<device name="" package="JJM">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="C" pad="C"/>
<connect gate="2" pin="NO1" pad="NO1"/>
<connect gate="2" pin="NO2" pad="NO2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JS-M1A*" prefix="K">
<description>&lt;b&gt;Automotive Ultra-Miniature Power Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61211_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="JS-M1A">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="-12V-4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="JSM1A-12V-4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P4554"/>
</technology>
<technology name="-12V-5">
<attribute name="MF" value=""/>
<attribute name="MPN" value="JSM1A-12V-5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P4555"/>
</technology>
<technology name="-9V-4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V-5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-12V-4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-12V5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-9V-4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-9V-5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JS-M1*" prefix="K">
<description>&lt;b&gt;Automotive Ultra-Miniature Power Relay&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61211_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="JS-M">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="C"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="-12V-4">
<attribute name="MF" value=""/>
<attribute name="MPN" value="JSM1-12V-4"/>
<attribute name="OC_FARNELL" value="910338"/>
<attribute name="OC_NEWARK" value="13P4552"/>
</technology>
<technology name="-12V-5">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="JSM1-12V-5"/>
<attribute name="OC_FARNELL" value="910351"/>
<attribute name="OC_NEWARK" value="14J1764"/>
</technology>
<technology name="-9V-4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V-5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-12V-4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-12V-5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-9V-4">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="F-9V-5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JT?-*" prefix="K">
<description>&lt;b&gt;COMPACT ECONOMICAL 30 AMP. RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61212_0000.pdf</description>
<gates>
<gate name="G$1" symbol="K"/>
<gate name="G$2" symbol="U"/>
</gates>
<devices>
<device name="" package="JT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$2" pin="O" pad="NC"/>
<connect gate="G$2" pin="P" pad="C"/>
<connect gate="G$2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC15V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N-PCB" package="JT-PCB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$2" pin="O" pad="NC"/>
<connect gate="G$2" pin="P" pad="C"/>
<connect gate="G$2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC15V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="N-TMB" package="JT-TMB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$2" pin="O" pad="NC"/>
<connect gate="G$2" pin="P" pad="C"/>
<connect gate="G$2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC15V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JT1A?-*" prefix="K">
<description>&lt;b&gt;COMPACT ECONOMICAL 30 AMP. RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61212_0000.pdf</description>
<gates>
<gate name="G$1" symbol="K"/>
<gate name="G$2" symbol="S"/>
</gates>
<devices>
<device name="" package="JT1A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$2" pin="P" pad="C"/>
<connect gate="G$2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC15V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-PCB" package="JT1A-PCB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$2" pin="P" pad="C"/>
<connect gate="G$2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC15V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-TMB" package="JT1A-TMB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$2" pin="P" pad="C"/>
<connect gate="G$2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="DC12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC15V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="DC9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQB*" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61604_0000.pdf</description>
<gates>
<gate name="1" symbol="PHOTOTRIAC"/>
</gates>
<devices>
<device name="" package="AQ-B">
<connects>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="DS1" pad="2"/>
<connect gate="1" pin="DS2" pad="1"/>
<connect gate="1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="1A-ZT3/6VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A1-T10/18VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A1-T18/30VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A1-T3/6VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A1-T7/14VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A1-ZT10/18VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A1-ZT18/30VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A1-ZT7/14VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A2-T10/18VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A2-T18/30VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A2-T3/6VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A2-T7/14VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A2-ZT10/18VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A2-ZT18/30VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A2-ZT3/6VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1A2-ZT7/14VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A1-T10/18VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A1-T18/30VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A1-T3/6VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A1-T7/14VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A1-ZT10/18VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A1-ZT18/30VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A1-ZT3/6VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A1-ZT7/14VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A2-T10/18VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A2-T18/30VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A2-T3/6VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A2-T7/14VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A2-ZT10/18VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A2-ZT18/30VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A2-ZT3/6VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2A2-ZT7/14VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CV13*" prefix="K">
<description>&lt;b&gt;AUTOMOTIVE LOW PROFILE MICRO-280 RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61214_0000.pdf</description>
<gates>
<gate name="G$2" symbol="U"/>
<gate name="G$1" symbol="K-DIODE"/>
</gates>
<devices>
<device name="" package="CV-MIRO-280">
<connects>
<connect gate="G$1" pin="+" pad="86"/>
<connect gate="G$1" pin="-" pad="85"/>
<connect gate="G$2" pin="O" pad="87A"/>
<connect gate="G$2" pin="P" pad="87"/>
<connect gate="G$2" pin="S" pad="30"/>
</connects>
<technologies>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ACV13012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="39M3504"/>
</technology>
<technology name="112">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="212">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CV33*" prefix="K">
<description>&lt;b&gt;AUTOMOTIVE LOW PROFILE MICRO-280 RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61214_0000.pdf</description>
<gates>
<gate name="G$1" symbol="K-DIODE"/>
<gate name="G$2" symbol="S"/>
</gates>
<devices>
<device name="" package="CV1A-MICRO-280">
<connects>
<connect gate="G$1" pin="+" pad="86"/>
<connect gate="G$1" pin="-" pad="85"/>
<connect gate="G$2" pin="P" pad="30"/>
<connect gate="G$2" pin="S" pad="87"/>
</connects>
<technologies>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ACV33012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="39M3505"/>
</technology>
<technology name="112">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="212">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RG1*" prefix="K">
<description>&lt;b&gt;HIGH FREQUENCY RELAYS WITH 1C AND 2C CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61302_0000.pdf</description>
<gates>
<gate name="G$1" symbol="K+-"/>
<gate name="G$2" symbol="U"/>
<gate name="G$3" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RG1">
<connects>
<connect gate="G$1" pin="+" pad="16"/>
<connect gate="G$1" pin="-" pad="15"/>
<connect gate="G$2" pin="O" pad="7"/>
<connect gate="G$2" pin="P" pad="4"/>
<connect gate="G$2" pin="S" pad="1"/>
<connect gate="G$3" pin="SH@1" pad="2"/>
<connect gate="G$3" pin="SH@2" pad="3"/>
<connect gate="G$3" pin="SH@3" pad="5"/>
<connect gate="G$3" pin="SH@4" pad="6"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-L" package="RG1">
<connects>
<connect gate="G$1" pin="+" pad="15"/>
<connect gate="G$1" pin="-" pad="16"/>
<connect gate="G$2" pin="O" pad="7"/>
<connect gate="G$2" pin="P" pad="4"/>
<connect gate="G$2" pin="S" pad="1"/>
<connect gate="G$3" pin="SH@1" pad="2"/>
<connect gate="G$3" pin="SH@2" pad="3"/>
<connect gate="G$3" pin="SH@3" pad="5"/>
<connect gate="G$3" pin="SH@4" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="T-L" package="RG1">
<connects>
<connect gate="G$1" pin="+" pad="15"/>
<connect gate="G$1" pin="-" pad="16"/>
<connect gate="G$2" pin="O" pad="7"/>
<connect gate="G$2" pin="P" pad="4"/>
<connect gate="G$2" pin="S" pad="1"/>
<connect gate="G$3" pin="SH@1" pad="2"/>
<connect gate="G$3" pin="SH@2" pad="3"/>
<connect gate="G$3" pin="SH@3" pad="5"/>
<connect gate="G$3" pin="SH@4" pad="6"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RG2*" prefix="K">
<description>&lt;b&gt;HIGH FREQUENCY RELAYS WITH 1C AND 2C CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61302_0000.pdf</description>
<gates>
<gate name="A" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
<gate name="S2" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RG2">
<connects>
<connect gate="1" pin="O" pad="7"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="A" pin="+" pad="16"/>
<connect gate="A" pin="-" pad="15"/>
<connect gate="S1" pin="SH@1" pad="2"/>
<connect gate="S1" pin="SH@2" pad="3"/>
<connect gate="S1" pin="SH@3" pad="5"/>
<connect gate="S1" pin="SH@4" pad="6"/>
<connect gate="S2" pin="SH@1" pad="9"/>
<connect gate="S2" pin="SH@2" pad="10"/>
<connect gate="S2" pin="SH@3" pad="12"/>
<connect gate="S2" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-L" package="RG2">
<connects>
<connect gate="1" pin="O" pad="7"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="A" pin="+" pad="15"/>
<connect gate="A" pin="-" pad="16"/>
<connect gate="S1" pin="SH@1" pad="2"/>
<connect gate="S1" pin="SH@2" pad="3"/>
<connect gate="S1" pin="SH@3" pad="5"/>
<connect gate="S1" pin="SH@4" pad="6"/>
<connect gate="S2" pin="SH@1" pad="9"/>
<connect gate="S2" pin="SH@2" pad="10"/>
<connect gate="S2" pin="SH@3" pad="12"/>
<connect gate="S2" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="T-L" package="RG2">
<connects>
<connect gate="1" pin="O" pad="7"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="A" pin="+" pad="15"/>
<connect gate="A" pin="-" pad="16"/>
<connect gate="S1" pin="SH@1" pad="2"/>
<connect gate="S1" pin="SH@2" pad="3"/>
<connect gate="S1" pin="SH@3" pad="5"/>
<connect gate="S1" pin="SH@4" pad="6"/>
<connect gate="S2" pin="SH@1" pad="9"/>
<connect gate="S2" pin="SH@2" pad="10"/>
<connect gate="S2" pin="SH@3" pad="12"/>
<connect gate="S2" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RG2-L-*" prefix="K">
<description>&lt;b&gt;HIGH FREQUENCY RELAYS WITH 1C AND 2C CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61302_0000.pdf</description>
<gates>
<gate name="-S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
<gate name="S2" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RG2">
<connects>
<connect gate="-S" pin="+" pad="16"/>
<connect gate="-S" pin="-" pad="15"/>
<connect gate="1" pin="O" pad="7"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="R" pin="+" pad="17"/>
<connect gate="R" pin="-" pad="18"/>
<connect gate="S1" pin="SH@1" pad="2"/>
<connect gate="S1" pin="SH@2" pad="3"/>
<connect gate="S1" pin="SH@3" pad="5"/>
<connect gate="S1" pin="SH@4" pad="6"/>
<connect gate="S2" pin="SH@1" pad="9"/>
<connect gate="S2" pin="SH@2" pad="10"/>
<connect gate="S2" pin="SH@3" pad="12"/>
<connect gate="S2" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RG2T-L2-*" prefix="K">
<description>&lt;b&gt;HIGH FREQUENCY RELAYS WITH 1C AND 2C CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61302_0000.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
<gate name="S2" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RG2">
<connects>
<connect gate="1" pin="O" pad="7"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="R" pin="+" pad="17"/>
<connect gate="R" pin="-" pad="18"/>
<connect gate="S" pin="+" pad="15"/>
<connect gate="S" pin="-" pad="16"/>
<connect gate="S1" pin="SH@1" pad="2"/>
<connect gate="S1" pin="SH@2" pad="3"/>
<connect gate="S1" pin="SH@3" pad="5"/>
<connect gate="S1" pin="SH@4" pad="6"/>
<connect gate="S2" pin="SH@1" pad="9"/>
<connect gate="S2" pin="SH@2" pad="10"/>
<connect gate="S2" pin="SH@3" pad="12"/>
<connect gate="S2" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RG1?-L2" prefix="K">
<description>&lt;b&gt;HIGH FREQUENCY RELAYS WITH 1C AND 2C CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61302_0000.pdf</description>
<gates>
<gate name="1" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
<gate name="R" symbol="K+-R"/>
<gate name="S" symbol="K+-S"/>
</gates>
<devices>
<device name="" package="RG1">
<connects>
<connect gate="1" pin="O" pad="7"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="R" pin="+" pad="16"/>
<connect gate="R" pin="-" pad="15"/>
<connect gate="S" pin="+" pad="17"/>
<connect gate="S" pin="-" pad="18"/>
<connect gate="S1" pin="SH@1" pad="2"/>
<connect gate="S1" pin="SH@2" pad="3"/>
<connect gate="S1" pin="SH@3" pad="5"/>
<connect gate="S1" pin="SH@4" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RG2T-L2*" prefix="K">
<description>&lt;b&gt;HIGH FREQUENCY RELAYS WITH 1C AND 2C CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61302_0000.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
<gate name="S2" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RG2">
<connects>
<connect gate="1" pin="O" pad="7"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="1"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="R" pin="+" pad="17"/>
<connect gate="R" pin="-" pad="18"/>
<connect gate="S" pin="+" pad="16"/>
<connect gate="S" pin="-" pad="15"/>
<connect gate="S1" pin="SH@1" pad="2"/>
<connect gate="S1" pin="SH@2" pad="3"/>
<connect gate="S1" pin="SH@3" pad="5"/>
<connect gate="S1" pin="SH@4" pad="6"/>
<connect gate="S2" pin="SH@1" pad="9"/>
<connect gate="S2" pin="SH@2" pad="10"/>
<connect gate="S2" pin="SH@3" pad="12"/>
<connect gate="S2" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RM2?*" prefix="K">
<description>&lt;b&gt;4 GHz 2 FORM C MICROWAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61305_0000.pdf</description>
<gates>
<gate name="A" symbol="K+-"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
<gate name="S2" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RM">
<connects>
<connect gate="1" pin="O" pad="8"/>
<connect gate="1" pin="P" pad="5"/>
<connect gate="1" pin="S" pad="2"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="14"/>
<connect gate="2" pin="S" pad="17"/>
<connect gate="A" pin="+" pad="9"/>
<connect gate="A" pin="-" pad="10"/>
<connect gate="S1" pin="SH@1" pad="3"/>
<connect gate="S1" pin="SH@2" pad="4"/>
<connect gate="S1" pin="SH@3" pad="6"/>
<connect gate="S1" pin="SH@4" pad="7"/>
<connect gate="S2" pin="SH@1" pad="12"/>
<connect gate="S2" pin="SH@2" pad="13"/>
<connect gate="S2" pin="SH@3" pad="15"/>
<connect gate="S2" pin="SH@4" pad="16"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-L" package="RM">
<connects>
<connect gate="1" pin="O" pad="8"/>
<connect gate="1" pin="P" pad="5"/>
<connect gate="1" pin="S" pad="2"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="14"/>
<connect gate="2" pin="S" pad="17"/>
<connect gate="A" pin="+" pad="10"/>
<connect gate="A" pin="-" pad="9"/>
<connect gate="S1" pin="SH@1" pad="3"/>
<connect gate="S1" pin="SH@2" pad="4"/>
<connect gate="S1" pin="SH@3" pad="6"/>
<connect gate="S1" pin="SH@4" pad="7"/>
<connect gate="S2" pin="SH@1" pad="12"/>
<connect gate="S2" pin="SH@2" pad="13"/>
<connect gate="S2" pin="SH@3" pad="15"/>
<connect gate="S2" pin="SH@4" pad="16"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RM2-L2*" prefix="K">
<description>&lt;b&gt;4 GHz 2 FORM C MICROWAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61305_0000.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
<gate name="S2" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RM2">
<connects>
<connect gate="1" pin="O" pad="8"/>
<connect gate="1" pin="P" pad="5"/>
<connect gate="1" pin="S" pad="2"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="14"/>
<connect gate="2" pin="S" pad="17"/>
<connect gate="R" pin="+" pad="18"/>
<connect gate="R" pin="-" pad="1"/>
<connect gate="S" pin="+" pad="9"/>
<connect gate="S" pin="-" pad="10"/>
<connect gate="S1" pin="SH@1" pad="3"/>
<connect gate="S1" pin="SH@2" pad="4"/>
<connect gate="S1" pin="SH@3" pad="6"/>
<connect gate="S1" pin="SH@4" pad="7"/>
<connect gate="S2" pin="SH@1" pad="12"/>
<connect gate="S2" pin="SH@2" pad="13"/>
<connect gate="S2" pin="SH@3" pad="15"/>
<connect gate="S2" pin="SH@4" pad="16"/>
</connects>
<technologies>
<technology name="-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP1-*" prefix="K">
<description>&lt;b&gt;LOW PROFILE HIGH FREQUENCY RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61306_0000.pdf</description>
<gates>
<gate name="2" symbol="U"/>
<gate name="1" symbol="K+-"/>
</gates>
<devices>
<device name="" package="RP">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="3"/>
<connect gate="2" pin="O" pad="4"/>
<connect gate="2" pin="P" pad="5"/>
<connect gate="2" pin="S" pad="6"/>
</connects>
<technologies>
<technology name="1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="RP1-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92B3783"/>
</technology>
<technology name="24V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="RP1-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9248"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="RP1-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="64K3170"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-1.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H-9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="H4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RX1?*" prefix="K">
<description>&lt;b&gt;SMALL MICRO WAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61307_0000.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="0" package="RX">
<connects>
<connect gate="1" pin="+" pad="7"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="SH@1" pad="9"/>
<connect gate="3" pin="SH@2" pad="10"/>
<connect gate="3" pin="SH@3" pad="12"/>
<connect gate="3" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="003">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="00H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="04H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="1" package="RX">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="7"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="SH@1" pad="9"/>
<connect gate="3" pin="SH@2" pad="10"/>
<connect gate="3" pin="SH@3" pad="12"/>
<connect gate="3" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="003">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="04H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RX12*" prefix="K">
<description>&lt;b&gt;SMALL MICRO WAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61307_0000.pdf</description>
<gates>
<gate name="1" symbol="+KS+KR-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RX2">
<connects>
<connect gate="1" pin="-" pad="1"/>
<connect gate="1" pin="R+" pad="6"/>
<connect gate="1" pin="S+" pad="7"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="3" pin="SH@1" pad="9"/>
<connect gate="3" pin="SH@2" pad="10"/>
<connect gate="3" pin="SH@3" pad="12"/>
<connect gate="3" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RA2?*" prefix="K">
<description>&lt;b&gt;MICROWAVE RELAY FOR ATTENUATOR CIRCUIT&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61308_0000.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="K-PIN"/>
<gate name="S1" symbol="SHIELD-3"/>
</gates>
<devices>
<device name="00A" package="RA">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="10"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="9"/>
<connect gate="3" pin="P" pad="8"/>
<connect gate="3" pin="S" pad="7"/>
<connect gate="4" pin="-" pad="10.1"/>
<connect gate="S1" pin="SH@1" pad="S3"/>
<connect gate="S1" pin="SH@2" pad="S2"/>
<connect gate="S1" pin="SH@3" pad="S1"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARA200A03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1235"/>
</technology>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="10A" package="RA-1COIL">
<connects>
<connect gate="1" pin="+" pad="10"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="9"/>
<connect gate="3" pin="P" pad="8"/>
<connect gate="3" pin="S" pad="7"/>
<connect gate="4" pin="-" pad="10.1"/>
<connect gate="S1" pin="SH@1" pad="S3"/>
<connect gate="S1" pin="SH@2" pad="S2"/>
<connect gate="S1" pin="SH@3" pad="S1"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="05">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="ARA210A05"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C4091"/>
</technology>
<technology name="06">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="ARA210A06"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C4092"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="ARA210A12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="64K3073"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4H">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="ARA210A4H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="64K3074"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RA220A*" prefix="K">
<description>&lt;b&gt;MICROWAVE RELAY FOR ATTENUATOR CIRCUIT&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61308_0000.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
<gate name="SH" symbol="SHIELD-2"/>
<gate name="P5" symbol="K-PIN"/>
<gate name="P6" symbol="K-PIN"/>
</gates>
<devices>
<device name="" package="RA-2COIL">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="8"/>
<connect gate="2" pin="S" pad="7"/>
<connect gate="P5" pin="-" pad="5.1"/>
<connect gate="P6" pin="-" pad="6.1"/>
<connect gate="R" pin="+" pad="1"/>
<connect gate="R" pin="-" pad="5"/>
<connect gate="S" pin="+" pad="10"/>
<connect gate="S" pin="-" pad="6"/>
<connect gate="SH" pin="SH@1" pad="S4"/>
<connect gate="SH" pin="SH@2" pad="S1"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARA220A03Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3559"/>
</technology>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARA220A05"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="15P8679"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARA220A12Z"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3560"/>
</technology>
<technology name="1H">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARA220A4HZ"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12N3561"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RE?*" prefix="K">
<description>&lt;b&gt;SMALL MICROWAVE RELAYS FOR BROADCASTING INDUSTRY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61310_0000.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="13" package="RE">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="7"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="S1" pin="SH@1" pad="9"/>
<connect gate="S1" pin="SH@2" pad="10"/>
<connect gate="S1" pin="SH@3" pad="12"/>
<connect gate="S1" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="ARE1303"/>
<attribute name="OC_FARNELL" value="1448347"/>
<attribute name="OC_NEWARK" value="64K3078"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE1306"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2917"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE1309"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="95M8248"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE1312"/>
<attribute name="OC_FARNELL" value="3773000"/>
<attribute name="OC_NEWARK" value="13P1245"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE1324"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2919"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE134H"/>
<attribute name="OC_FARNELL" value="3772998"/>
<attribute name="OC_NEWARK" value="13P1246"/>
</technology>
</technologies>
</device>
<device name="13A" package="RE-SMD">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="7"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="S1" pin="SH@1" pad="9"/>
<connect gate="S1" pin="SH@2" pad="10"/>
<connect gate="S1" pin="SH@3" pad="12"/>
<connect gate="S1" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE13A03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="71M0380"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE13A06"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2902"/>
</technology>
<technology name="09">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE13A09"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2904"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE13A12"/>
<attribute name="OC_FARNELL" value="3773036"/>
<attribute name="OC_NEWARK" value="13P1241"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE13A24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2909"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARE13A4H"/>
<attribute name="OC_FARNELL" value="3773024"/>
<attribute name="OC_NEWARK" value="11N2913"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RK1?-*" prefix="K">
<description>&lt;b&gt;1.5 GHz MICROWAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61311_0000.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="S" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RK1A">
<connects>
<connect gate="1" pin="+" pad="7"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="S" pin="SH@1" pad="9"/>
<connect gate="S" pin="SH@2" pad="10"/>
<connect gate="S" pin="SH@3" pad="12"/>
<connect gate="S" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RK1-12V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P6876"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RK1-24V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P6877"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RK1-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P6878"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RK1-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P6879"/>
</technology>
<technology name="6V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="RK1-6V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9196"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R" package="RK1A">
<connects>
<connect gate="1" pin="+" pad="7"/>
<connect gate="1" pin="-" pad="1"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="S" pin="SH@1" pad="9"/>
<connect gate="S" pin="SH@2" pad="10"/>
<connect gate="S" pin="SH@3" pad="12"/>
<connect gate="S" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-L" package="RK1A">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="7"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="S" pin="SH@1" pad="9"/>
<connect gate="S" pin="SH@2" pad="10"/>
<connect gate="S" pin="SH@3" pad="12"/>
<connect gate="S" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RK1-L-4.5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N5893"/>
</technology>
<technology name="5V">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="RK1-L-5V"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C9186"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R-L" package="RK1A">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="7"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="S" pin="SH@1" pad="9"/>
<connect gate="S" pin="SH@2" pad="10"/>
<connect gate="S" pin="SH@3" pad="12"/>
<connect gate="S" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4.5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RK1?-L2*" prefix="K">
<description>&lt;b&gt;1.5 GHz MICROWAVE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61311_0000.pdf</description>
<gates>
<gate name="1" symbol="+KS+KR-"/>
<gate name="2" symbol="U"/>
<gate name="S1" symbol="SHIELD-4"/>
</gates>
<devices>
<device name="" package="RKL2">
<connects>
<connect gate="1" pin="-" pad="1"/>
<connect gate="1" pin="R+" pad="7"/>
<connect gate="1" pin="S+" pad="6"/>
<connect gate="2" pin="O" pad="14"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="8"/>
<connect gate="S1" pin="SH@1" pad="9"/>
<connect gate="S1" pin="SH@2" pad="10"/>
<connect gate="S1" pin="SH@3" pad="12"/>
<connect gate="S1" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="RK1-L2-12V"/>
<attribute name="OC_FARNELL" value="1616207"/>
<attribute name="OC_NEWARK" value="10C9189"/>
</technology>
</technologies>
</device>
<device name="R" package="RKL2">
<connects>
<connect gate="1" pin="-" pad="1"/>
<connect gate="1" pin="R+" pad="7"/>
<connect gate="1" pin="S+" pad="6"/>
<connect gate="2" pin="O" pad="8"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="S1" pin="SH@1" pad="9"/>
<connect gate="S1" pin="SH@2" pad="10"/>
<connect gate="S1" pin="SH@3" pad="12"/>
<connect gate="S1" pin="SH@4" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQ?" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61601_0000.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOTRIAC"/>
</gates>
<devices>
<device name="2A2-ZP3" package="AQ1">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="2"/>
<connect gate="G$1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQ2A2-ZP3/28VDC"/>
<attribute name="OC_FARNELL" value="1163552"/>
<attribute name="OC_NEWARK" value="13P1232"/>
</technology>
</technologies>
</device>
<device name="2A2-J-ZP3" package="AQ1-FLAT">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="2"/>
<connect gate="G$1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQ2A2-ZP3/28VDC"/>
<attribute name="OC_FARNELL" value="1163552"/>
<attribute name="OC_NEWARK" value="13P1232"/>
</technology>
</technologies>
</device>
<device name="5A2-ZP3" package="AQ1-M">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="2"/>
<connect gate="G$1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQ5A2-ZP3/28VDC"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1233"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQ*" prefix="K">
<description>&lt;b&gt;SOLID STATE RELAY&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/..  en_ds_61601_0000.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS-DC"/>
</gates>
<devices>
<device name="" package="AQ1">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="2"/>
<connect gate="G$1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="1AD2-3">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="AQ1AD2-3/28VDC"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="10C4052"/>
</technology>
<technology name="2AD1-3">
<attribute name="MF" value=""/>
<attribute name="MPN" value="AQ2AD1-3/28VDC"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1229"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ?*" prefix="K">
<description>&lt;b&gt;SMD RELAYS WITH 5GHz CAPABILITIES&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61313_0000.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="20" package="RJ">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="3"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="2"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="9"/>
<connect gate="3" pin="P" pad="7"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ2003"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2927"/>
</technology>
<technology name="12">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="ARJ2012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="81C8602"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ2024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2928"/>
</technology>
<technology name="4H">
<attribute name="MF" value="AROMAT/ MATSUSHITA"/>
<attribute name="MPN" value="ARJ204H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="63H2424"/>
</technology>
</technologies>
</device>
<device name="20A" package="RJ-SMD">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="3"/>
<connect gate="2" pin="O" pad="10"/>
<connect gate="2" pin="P" pad="2"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="9"/>
<connect gate="3" pin="P" pad="7"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ20A03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2921"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ20A12"/>
<attribute name="OC_FARNELL" value="8928207"/>
<attribute name="OC_NEWARK" value="13P1247"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ20A24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2924"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ20A4H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1248"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ22?*" prefix="K">
<description>&lt;b&gt;SMD RELAYS WITH 5GHz CAPABILITIES&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61313_0000.pdf</description>
<gates>
<gate name="S" symbol="K+-S"/>
<gate name="R" symbol="K+-R"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="A" package="RJ-SMD">
<connects>
<connect gate="1" pin="O" pad="10"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="5"/>
<connect gate="R" pin="+" pad="8"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="3"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ22A03"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2929"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ22A12"/>
<attribute name="OC_FARNELL" value="9008446"/>
<attribute name="OC_NEWARK" value="13P1249"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ22A24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2932"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ22A4H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13P1250"/>
</technology>
</technologies>
</device>
<device name="" package="RJ">
<connects>
<connect gate="1" pin="O" pad="10"/>
<connect gate="1" pin="P" pad="2"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="9"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="5"/>
<connect gate="R" pin="+" pad="8"/>
<connect gate="R" pin="-" pad="6"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="3"/>
</connects>
<technologies>
<technology name="03">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ2203"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2935"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ2212"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2936"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ2224"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2937"/>
</technology>
<technology name="4H">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ARJ224H"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11N2938"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SF2-*" prefix="K">
<description>&lt;b&gt;POLARISED, MONOSTABLE RELAY WITH FORCIBLY GUIDED CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61404_0001.pdf</description>
<gates>
<gate name="S" symbol="K+-"/>
<gate name="1" symbol="O"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
</gates>
<devices>
<device name="" package="SF2">
<connects>
<connect gate="1" pin="O" pad="5"/>
<connect gate="1" pin="P" pad="6"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="3" pin="P" pad="7"/>
<connect gate="3" pin="S" pad="8"/>
<connect gate="4" pin="P" pad="10"/>
<connect gate="4" pin="S" pad="9"/>
<connect gate="S" pin="+" pad="1"/>
<connect gate="S" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="SF2-12V"/>
<attribute name="OC_FARNELL" value="625875"/>
<attribute name="OC_NEWARK" value="68C0655"/>
</technology>
<technology name="18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="21V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SF2-24V"/>
<attribute name="OC_FARNELL" value="1124064"/>
<attribute name="OC_NEWARK" value="31M0404"/>
</technology>
<technology name="36V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="60V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SF3-*" prefix="K">
<description>&lt;b&gt;POLARISED, MONOSTABLE RELAY WITH FORCIBLY GUIDED CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61404_0001.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="S"/>
</gates>
<devices>
<device name="" package="SF2">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="2"/>
<connect gate="2" pin="O" pad="5"/>
<connect gate="2" pin="P" pad="6"/>
<connect gate="3" pin="P" pad="7"/>
<connect gate="3" pin="S" pad="8"/>
<connect gate="4" pin="P" pad="10"/>
<connect gate="4" pin="S" pad="9"/>
<connect gate="5" pin="P" pad="11"/>
<connect gate="5" pin="S" pad="12"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="21V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="36V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="60V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SF4D-*" prefix="K">
<description>&lt;b&gt;POLARISED, MONOSTABLE RELAY WITH FORCIBLY GUIDED DOUBLE CONTACTS&lt;/b&gt; NAiS&lt;p&gt;
Source: http://www.mew-europe.com/.. en_ds_61407_0002.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="O"/>
<gate name="6" symbol="S"/>
<gate name="7" symbol="O"/>
<gate name="8" symbol="O"/>
<gate name="9" symbol="S"/>
</gates>
<devices>
<device name="" package="SF4D">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="2"/>
<connect gate="2" pin="O" pad="5"/>
<connect gate="2" pin="P" pad="6"/>
<connect gate="3" pin="P" pad="7"/>
<connect gate="3" pin="S" pad="8"/>
<connect gate="4" pin="P" pad="10"/>
<connect gate="4" pin="S" pad="9"/>
<connect gate="5" pin="O" pad="12"/>
<connect gate="5" pin="P" pad="11"/>
<connect gate="6" pin="P" pad="14"/>
<connect gate="6" pin="S" pad="13"/>
<connect gate="7" pin="O" pad="16"/>
<connect gate="7" pin="P" pad="15"/>
<connect gate="8" pin="O" pad="17"/>
<connect gate="8" pin="P" pad="18"/>
<connect gate="9" pin="P" pad="19"/>
<connect gate="9" pin="S" pad="20"/>
</connects>
<technologies>
<technology name="12V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="18V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="21V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="36V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="60V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="S?*" prefix="K">
<description>&lt;b&gt;Low Height Type Solid State Relays&lt;/b&gt; SHARP&lt;p&gt;
Source: 162574-da-01-en-S202T02_Solid_State_Relais.pdf
Source: http://sharp-world.com .. s102s11_e.pdf</description>
<gates>
<gate name="1" symbol="PHOTOTRIAC"/>
</gates>
<devices>
<device name="101T" package="S102T0X">
<connects>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="DS1" pad="1"/>
<connect gate="1" pin="DS2" pad="2"/>
<connect gate="1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="02">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="102T" package="S102T0X">
<connects>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="DS1" pad="1"/>
<connect gate="1" pin="DS2" pad="2"/>
<connect gate="1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="01">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="02">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="202S" package="S2XXEX">
<connects>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="DS1" pad="2"/>
<connect gate="1" pin="DS2" pad="1"/>
<connect gate="1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="11">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="102S" package="S2XXEX">
<connects>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="DS1" pad="1"/>
<connect gate="1" pin="DS2" pad="2"/>
<connect gate="1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="11">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="102S01" package="S102S01">
<connects>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="DS1" pad="1"/>
<connect gate="1" pin="DS2" pad="2"/>
<connect gate="1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="202S01" package="S102S01">
<connects>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="DS1" pad="1"/>
<connect gate="1" pin="DS2" pad="2"/>
<connect gate="1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="S202S01F"/>
<attribute name="OC_FARNELL" value="1618474"/>
<attribute name="OC_NEWARK" value="14N9587"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="S2*" prefix="K">
<description>&lt;b&gt;SIP Type SSR for Medium Power Control&lt;/b&gt; SHARP&lt;p&gt;
Source: 168149-da-01-en-Solid_State_Relais_S_202_SE1_SE2.pdf&lt;br&gt;</description>
<gates>
<gate name="1" symbol="PHOTOTRIAC"/>
</gates>
<devices>
<device name="" package="S2XXEX">
<connects>
<connect gate="1" pin="A" pad="3"/>
<connect gate="1" pin="DS1" pad="1"/>
<connect gate="1" pin="DS2" pad="2"/>
<connect gate="1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="02SE1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="02SE2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="16SE1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="16SE2">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PE*" prefix="K">
<description>&lt;b&gt;Miniature PCB Relay 1 pole 5 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5807.pdf&lt;br&gt;
Miniature PCB Relay bistable 1pole 5 A, polarized bistable version&lt;br&gt;
Source: http://www.schrack.com/.. 5808.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="PE">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A03">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="A24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SR2Y5*" prefix="K">
<description>&lt;b&gt;Safety Relay 2 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5809.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="SR2Y">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="018">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="021">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="036">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="040">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="080">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SR2X5*" prefix="K">
<description>&lt;b&gt;Safety Relay 2 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5809.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="S"/>
</gates>
<devices>
<device name="" package="SR2X">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="21"/>
<connect gate="2" pin="P" pad="22"/>
<connect gate="3" pin="P" pad="14"/>
<connect gate="3" pin="S" pad="13"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="018">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="021">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="036">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="040">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="080">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RE03*" prefix="K">
<description>&lt;b&gt;Miniature PCB Relay 1 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5812.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="RE-SCHRACK">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RE030005"/>
<attribute name="OC_FARNELL" value="515838"/>
<attribute name="OC_NEWARK" value="52F908"/>
</technology>
<technology name="0006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RE030006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="92C1858"/>
</technology>
<technology name="0012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RE030012"/>
<attribute name="OC_FARNELL" value="515840"/>
<attribute name="OC_NEWARK" value="17M1743"/>
</technology>
<technology name="0024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RE030024"/>
<attribute name="OC_FARNELL" value="515851"/>
<attribute name="OC_NEWARK" value="52F910"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1629023"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RE032005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="97K8812"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RE032012"/>
<attribute name="OC_FARNELL" value="9659684"/>
<attribute name="OC_NEWARK" value="97K8813"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RE032024"/>
<attribute name="OC_FARNELL" value="9659692"/>
<attribute name="OC_NEWARK" value="97K8814"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SR6-D4*" prefix="K">
<description>&lt;b&gt;Safety Relay 4 pole 8 A&lt;/b&gt; SCHRACK&lt;p&gt;
2 N/O contact and 2 N/C contact&lt;br&gt;
Source: http://www.schrack.com/.. 5814.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="O"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="S"/>
</gates>
<devices>
<device name="" package="SR6-D">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="12"/>
<connect gate="3" pin="O" pad="21"/>
<connect gate="3" pin="P" pad="22"/>
<connect gate="4" pin="P" pad="34"/>
<connect gate="4" pin="S" pad="33"/>
<connect gate="5" pin="P" pad="44"/>
<connect gate="5" pin="S" pad="43"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SR6D4012"/>
<attribute name="OC_FARNELL" value="1770622"/>
<attribute name="OC_NEWARK" value="51R7440"/>
</technology>
<technology name="018">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="021">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SR6D4024"/>
<attribute name="OC_FARNELL" value="1770623"/>
<attribute name="OC_NEWARK" value="51R7441"/>
</technology>
<technology name="036">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="040">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="085">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SR6D4110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R7721"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SR6-M4*" prefix="K">
<description>&lt;b&gt;Safety Relay 4 pole 8 A&lt;/b&gt; SCHRACK&lt;p&gt;
3 N/O contact and 1 N/C contact&lt;br&gt;
Source: http://www.schrack.com/.. 5814.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="O"/>
</gates>
<devices>
<device name="" package="SR6-M">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="14"/>
<connect gate="2" pin="S" pad="13"/>
<connect gate="3" pin="P" pad="34"/>
<connect gate="3" pin="S" pad="33"/>
<connect gate="4" pin="P" pad="44"/>
<connect gate="4" pin="S" pad="43"/>
<connect gate="5" pin="O" pad="21"/>
<connect gate="5" pin="P" pad="22"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SR6M4012"/>
<attribute name="OC_FARNELL" value="1770624"/>
<attribute name="OC_NEWARK" value="51R7442"/>
</technology>
<technology name="018">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="021">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="SR6M4024"/>
<attribute name="OC_FARNELL" value="1770625"/>
<attribute name="OC_NEWARK" value="51R7443"/>
</technology>
<technology name="036">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="040">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="085">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SNR?*" prefix="K">
<description>&lt;b&gt;Slim PCB Relay 1 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5815.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="0" package="SNR-V">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5" package="SNR-H">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SN*" prefix="K">
<description>&lt;b&gt;Slim PCB Relay 1 pole 6 A&lt;/b&gt; SCHRACK&lt;p&gt;
Source: http://www.schrack.com/.. 5815.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="R6" package="SNR-H6">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="8048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="R1" package="SNR-V1">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RY?1*" prefix="K">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5817.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="2" package="RY-II">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY210005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3762"/>
</technology>
<technology name="0006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY210006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3763"/>
</technology>
<technology name="0012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY210012"/>
<attribute name="OC_FARNELL" value="1652614"/>
<attribute name="OC_NEWARK" value="18C5386"/>
</technology>
<technology name="0024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY210024"/>
<attribute name="OC_FARNELL" value="1652615"/>
<attribute name="OC_NEWARK" value="17M1790"/>
</technology>
<technology name="0048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY210048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3765"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY211005"/>
<attribute name="OC_FARNELL" value="1629032"/>
<attribute name="OC_NEWARK" value="16R6445"/>
</technology>
<technology name="1006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="4-1393224-3"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13H3089"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY211012R"/>
<attribute name="OC_FARNELL" value="1629033"/>
<attribute name="OC_NEWARK" value="03P2440"/>
</technology>
<technology name="1024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY211024"/>
<attribute name="OC_FARNELL" value="1629034"/>
<attribute name="OC_NEWARK" value="08H3766"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY211048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8018"/>
</technology>
<technology name="2005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY212005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8019"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY212012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8020"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY212024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8021"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY213012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6446"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY213024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="59P3026"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5" package="RY-II">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="6" package="RY-II">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY610005"/>
<attribute name="OC_FARNELL" value="515863"/>
<attribute name="OC_NEWARK" value="48F5539"/>
</technology>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY610012"/>
<attribute name="OC_FARNELL" value="515875"/>
<attribute name="OC_NEWARK" value="52F1002"/>
</technology>
<technology name="0024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY610024"/>
<attribute name="OC_FARNELL" value="515887"/>
<attribute name="OC_NEWARK" value="52F1003"/>
</technology>
<technology name="0048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY610048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3773"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY611005"/>
<attribute name="OC_FARNELL" value="9659706"/>
<attribute name="OC_NEWARK" value="97K9204"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY611012"/>
<attribute name="OC_FARNELL" value="9659714"/>
<attribute name="OC_NEWARK" value="97K9205"/>
</technology>
<technology name="1024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY611024"/>
<attribute name="OC_FARNELL" value="9659722"/>
<attribute name="OC_NEWARK" value="29C5433"/>
</technology>
<technology name="1048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY611048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3777"/>
</technology>
<technology name="2005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY612005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8046"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY612012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96B4867"/>
</technology>
<technology name="2024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY612024"/>
<attribute name="OC_FARNELL" value="1703736"/>
<attribute name="OC_NEWARK" value="89C3213"/>
</technology>
<technology name="2048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY612048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="73C7516"/>
</technology>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY613005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6452"/>
</technology>
<technology name="3006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY613012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="29M8966"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY613024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8052"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="RY-II">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RY?3*" prefix="K">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5817.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="2" package="RY-II1">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY230048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8022"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5" package="RY-II1">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY530005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8023"/>
</technology>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY530006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8024"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY530012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8025"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY530024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8027"/>
</technology>
<technology name="0048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RY530048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3770"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY531005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8029"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY531012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6447"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY531024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6448"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY532012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8031"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY532024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6449"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY533012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8033"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY533024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6450"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RY900016(RY533048)"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M8055"/>
</technology>
</technologies>
</device>
<device name="6" package="RY-II1">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="A" package="RY-II1">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RYA30005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7996"/>
</technology>
<technology name="0006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RYA30006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3758"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RYA30012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="89M6563"/>
</technology>
<technology name="0024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RYA30024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="52F1005"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RYA31005"/>
<attribute name="OC_FARNELL" value="9659730"/>
<attribute name="OC_NEWARK" value="97K9200"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RYA31012"/>
<attribute name="OC_FARNELL" value="9659749"/>
<attribute name="OC_NEWARK" value="97K9201"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RYA31024"/>
<attribute name="OC_FARNELL" value="9659757"/>
<attribute name="OC_NEWARK" value="97K9202"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RYA31048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6440"/>
</technology>
<technology name="2005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RYA32005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3760"/>
</technology>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RYA32012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6441"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="3048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT?1*" prefix="K">
<description>&lt;b&gt;Power PCB Relayl&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 12 / 16 A, DC- or AC-coi&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="1" package="RT-C/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="4005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT114005"/>
<attribute name="OC_FARNELL" value="1629035"/>
<attribute name="OC_NEWARK" value="03P2411"/>
</technology>
<technology name="4006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT114006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="07H3171"/>
</technology>
<technology name="4012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT114012"/>
<attribute name="OC_FARNELL" value="1629036"/>
<attribute name="OC_NEWARK" value="03P2412"/>
</technology>
<technology name="4024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT114024"/>
<attribute name="OC_FARNELL" value="1629038"/>
<attribute name="OC_NEWARK" value="03P2413"/>
</technology>
<technology name="4048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT114048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3723"/>
</technology>
<technology name="4060">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT114060"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6359"/>
</technology>
<technology name="4110">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT114110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3725"/>
</technology>
<technology name="4524">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT114524"/>
<attribute name="OC_FARNELL" value="1629040"/>
<attribute name="OC_NEWARK" value="03P2415"/>
</technology>
<technology name="4615">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT114615"/>
<attribute name="OC_FARNELL" value="1629041"/>
<attribute name="OC_NEWARK" value="03P2416"/>
</technology>
<technology name="4730">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT114730"/>
<attribute name="OC_FARNELL" value="1629042"/>
<attribute name="OC_NEWARK" value="03P2417"/>
</technology>
</technologies>
</device>
<device name="2" package="RT-C/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="4005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT214006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3734"/>
</technology>
<technology name="4012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT214012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7937"/>
</technology>
<technology name="4024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT214024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3735"/>
</technology>
<technology name="4048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT214048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6362"/>
</technology>
<technology name="4060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4110">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT214110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6363"/>
</technology>
<technology name="4524">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT214524"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="50H8104"/>
</technology>
<technology name="4615">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT214615"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="93B6578"/>
</technology>
<technology name="4730">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT214730"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3736"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT31*" prefix="K">
<description>&lt;b&gt;Power PCB Relayl&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 12 / 16 A, DC- or AC-coi&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U-X2"/>
</gates>
<devices>
<device name="" package="RT-C/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="4005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314005"/>
<attribute name="OC_FARNELL" value="1629043"/>
<attribute name="OC_NEWARK" value="03P2418"/>
</technology>
<technology name="4006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314012"/>
<attribute name="OC_FARNELL" value="1629044"/>
<attribute name="OC_NEWARK" value="03P2419"/>
</technology>
<technology name="4024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT314024"/>
<attribute name="OC_FARNELL" value="1629045"/>
<attribute name="OC_NEWARK" value="36K2037"/>
</technology>
<technology name="4048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314048"/>
<attribute name="OC_FARNELL" value="1629046"/>
<attribute name="OC_NEWARK" value="03P2421"/>
</technology>
<technology name="4060">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314060"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6367"/>
</technology>
<technology name="4110">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7956"/>
</technology>
<technology name="4524">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314524"/>
<attribute name="OC_FARNELL" value="1629047"/>
<attribute name="OC_NEWARK" value="03P2422"/>
</technology>
<technology name="4615">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT314615"/>
<attribute name="OC_FARNELL" value="1629048"/>
<attribute name="OC_NEWARK" value="08H3745"/>
</technology>
<technology name="4730">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314730"/>
<attribute name="OC_FARNELL" value="1629051"/>
<attribute name="OC_NEWARK" value="03P2424"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT?*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 12 / 16 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="B3" package="RT-N/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="4005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RTB34005F"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3696"/>
</technology>
<technology name="4006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RTB34012"/>
<attribute name="OC_FARNELL" value="9865071"/>
<attribute name="OC_NEWARK" value="48M7873"/>
</technology>
<technology name="4024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RTB34024F"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="35K3224"/>
</technology>
<technology name="4048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4730">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RTB34730"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7874"/>
</technology>
</technologies>
</device>
<device name="C3" package="RT-N/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="4005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="184" package="RT-N/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT184005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3730"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT184012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3731"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT184024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3733"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTD3*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 12 / 16 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5819.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S-X2"/>
</gates>
<devices>
<device name="" package="RT-N/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="4005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RTD34005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="93B4654"/>
</technology>
<technology name="4006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RTD34012F"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="36K3470"/>
</technology>
<technology name="4024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RTD34024F"/>
<attribute name="OC_FARNELL" value="9850961"/>
<attribute name="OC_NEWARK" value="34K0187"/>
</technology>
<technology name="4048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RTD34048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3709"/>
</technology>
<technology name="4060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="4615">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RTD34615"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48F1293"/>
</technology>
<technology name="4730">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RTD34730"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="85C1167"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT?F*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
bistable 1 pole 16 A, polarized bistable version&lt;br&gt;
Source: http://www.schrack.com/.. 5821.pdf</description>
<gates>
<gate name="1" symbol="+KS+KR-"/>
<gate name="2" symbol="U-X2"/>
</gates>
<devices>
<device name="314" package="RT1-BI">
<connects>
<connect gate="1" pin="-" pad="A3"/>
<connect gate="1" pin="R+" pad="A2"/>
<connect gate="1" pin="S+" pad="A1"/>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314F05"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7949"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314F12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="26M2701"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314F24"/>
<attribute name="OC_FARNELL" value="1175084"/>
<attribute name="OC_NEWARK" value="31M5918"/>
</technology>
</technologies>
</device>
<device name="D14" package="RT1-BI">
<connects>
<connect gate="1" pin="-" pad="A3"/>
<connect gate="1" pin="R+" pad="A2"/>
<connect gate="1" pin="S+" pad="A1"/>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT?A*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
bistable 1 pole 16 A, polarized bistable version&lt;br&gt;
Source: http://www.schrack.com/.. 5821.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U-X2"/>
</gates>
<devices>
<device name="314" package="RT1-BI">
<connects>
<connect gate="1" pin="+" pad="A1"/>
<connect gate="1" pin="-" pad="A2"/>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT314A06"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7945"/>
</technology>
<technology name="12">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT314A12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3738"/>
</technology>
<technology name="24">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT314A24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3739"/>
</technology>
</technologies>
</device>
<device name="D14" package="RT1-BI">
<connects>
<connect gate="1" pin="+" pad="A1"/>
<connect gate="1" pin="-" pad="A2"/>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT174*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
sensitive 1 pole 10 A, highly sensitive version&lt;br&gt;
Source: http://www.schrack.com/.. 5822.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="RT-C/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT174005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7931"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT174012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3728"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT174024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3729"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PT5*" prefix="K">
<description>&lt;b&gt;Miniature Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 12 A, 3 pole 10 A or 4 pole 6 A DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5823.pdf&lt;br&gt;
Socked 78604 Source: http://www.schrack.com/.. 5836.pdf&lt;br&gt;</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
<gate name="5" symbol="U"/>
</gates>
<devices>
<device name="" package="PT-4">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
<connect gate="4" pin="O" pad="32"/>
<connect gate="4" pin="P" pad="31"/>
<connect gate="4" pin="S" pad="34"/>
<connect gate="5" pin="O" pad="42"/>
<connect gate="5" pin="P" pad="41"/>
<connect gate="5" pin="S" pad="44"/>
</connects>
<technologies>
<technology name="71506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71524">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="PT571524"/>
<attribute name="OC_FARNELL" value="3072836"/>
<attribute name="OC_NEWARK" value="08J0830"/>
</technology>
<technology name="71548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71560">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71615">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="PT571615"/>
<attribute name="OC_FARNELL" value="3072990"/>
<attribute name="OC_NEWARK" value="85H0667"/>
</technology>
<technology name="71730">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="PT571730"/>
<attribute name="OC_FARNELL" value="3073014"/>
<attribute name="OC_NEWARK" value="18J8266"/>
</technology>
<technology name="71R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81560">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-78604" package="PT78604">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
<connect gate="4" pin="O" pad="32"/>
<connect gate="4" pin="P" pad="31"/>
<connect gate="4" pin="S" pad="34"/>
<connect gate="5" pin="O" pad="42"/>
<connect gate="5" pin="P" pad="41"/>
<connect gate="5" pin="S" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PT2*" prefix="K">
<description>&lt;b&gt;Miniature Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 12 A DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5823.pdf&lt;br&gt;
Socked 78602 Source: http://www.schrack.com/.. 5836.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="PT-2">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="42"/>
<connect gate="3" pin="P" pad="41"/>
<connect gate="3" pin="S" pad="44"/>
</connects>
<technologies>
<technology name="71506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71560">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71615">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="PT271615"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="96H9720"/>
</technology>
<technology name="71730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81560">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-78602" package="PT78602">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="42"/>
<connect gate="3" pin="P" pad="41"/>
<connect gate="3" pin="S" pad="44"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PT3*" prefix="K">
<description>&lt;b&gt;Miniature Relay&lt;/b&gt; SCHRACK&lt;p&gt;
3 pole 10 A DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5823.pdf&lt;br&gt;
Socked 78603 Source: http://www.schrack.com/.. 5836.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="" package="PT-3">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
<connect gate="4" pin="O" pad="32"/>
<connect gate="4" pin="P" pad="31"/>
<connect gate="4" pin="S" pad="34"/>
</connects>
<technologies>
<technology name="71506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71560">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71R60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="71T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81560">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81R60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="81T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-78603" package="PT78603">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
<connect gate="4" pin="O" pad="32"/>
<connect gate="4" pin="P" pad="31"/>
<connect gate="4" pin="S" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT33*" prefix="K">
<description>&lt;b&gt;Power PCB Relay Inrush &lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A, for inrush peak currents up to 80 A&lt;br&gt;
Source: http://www.schrack.com/.. 5825.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S-X2"/>
</gates>
<devices>
<device name="" package="RT-N/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="K012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT33K012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7964"/>
</technology>
<technology name="K024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT33K024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7965"/>
</technology>
<technology name="K048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT33K048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6370"/>
</technology>
<technology name="K060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="L012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT33L012"/>
<attribute name="OC_FARNELL" value="1770614"/>
<attribute name="OC_NEWARK" value="74R4452"/>
</technology>
<technology name="L024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT33L024"/>
<attribute name="OC_FARNELL" value="1770616"/>
<attribute name="OC_NEWARK" value="74R4453"/>
</technology>
<technology name="L048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT33L048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6377"/>
</technology>
<technology name="L060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTH84*" prefix="K">
<description>&lt;b&gt;Power PCB Relay 105°C sensitive&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 10 A, high-temperature version&lt;br&gt;
Source: http://www.schrack.com/.. 5828.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S-X2"/>
</gates>
<devices>
<device name="" package="RT-N/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RM?*" prefix="K">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
3 pole 10 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5829.pdf&lt;br&gt;
Socket with PCB terminals&lt;br&gt;
Source: http://www.schrack.com/.. 5841.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
<gate name="4" symbol="U"/>
</gates>
<devices>
<device name="3" package="RM-2/3/7">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
<connect gate="4" pin="O" pad="32"/>
<connect gate="4" pin="P" pad="31"/>
<connect gate="4" pin="S" pad="34"/>
</connects>
<technologies>
<technology name="506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="900">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="V00">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="7" package="RM-2/3/7">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
<connect gate="4" pin="O" pad="32"/>
<connect gate="4" pin="P" pad="31"/>
<connect gate="4" pin="S" pad="34"/>
</connects>
<technologies>
<technology name="506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="900">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="V00">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="78702" package="RM78702">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
<connect gate="4" pin="O" pad="32"/>
<connect gate="4" pin="P" pad="31"/>
<connect gate="4" pin="S" pad="34"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RM78702"/>
<attribute name="OC_FARNELL" value="1652632"/>
<attribute name="OC_NEWARK" value="36K3468"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RM2*" prefix="K">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 16 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5829.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="RM-2">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="32"/>
<connect gate="3" pin="P" pad="31"/>
<connect gate="3" pin="S" pad="34"/>
</connects>
<technologies>
<technology name="506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="900">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="V00">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTH14*" prefix="K">
<description>&lt;b&gt;Power PCB Relay 105°C 16A&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A, high-temperature version&lt;br&gt;
Source: http://www.schrack.com/.. 5831.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U-X2"/>
</gates>
<devices>
<device name="" package="RT-C/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RTH14012"/>
<attribute name="OC_FARNELL" value="1629018"/>
<attribute name="OC_NEWARK" value="03P2408"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="7-1415025-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H4440"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RTH34*" prefix="K">
<description>&lt;b&gt;Power PCB Relay 105°C 16A&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A, high-temperature version&lt;br&gt;
Source: http://www.schrack.com/.. 5831.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S-X2"/>
</gates>
<devices>
<device name="" package="RT-N/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RTH34012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="45K1533"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RTH34024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="45K1534"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RM6*" prefix="K">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
3 pole 10 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5832.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
</gates>
<devices>
<device name="" package="RM-5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
<connect gate="4" pin="P" pad="31"/>
<connect gate="4" pin="S" pad="34"/>
</connects>
<technologies>
<technology name="07506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07524">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RM607524"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7685"/>
</technology>
<technology name="07548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07560">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07730">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RM607730"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="03M2867"/>
</technology>
<technology name="07900">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07V00">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RM5*" prefix="K">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 16 A, DC- or AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5832.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
</gates>
<devices>
<device name="" package="RM-6">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="P" pad="31"/>
<connect gate="3" pin="S" pad="34"/>
</connects>
<technologies>
<technology name="07506">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07512">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07548">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07560">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07900">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07R60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07T30">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="07V00">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?1*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U-X2"/>
</gates>
<devices>
<device name="3" package="RT-C/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP310005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7769"/>
</technology>
<technology name="0006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP310006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3568"/>
</technology>
<technology name="0012">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="RP310012."/>
<attribute name="OC_FARNELL" value="388294"/>
<attribute name="OC_NEWARK" value="87H7751"/>
</technology>
<technology name="0024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP310024"/>
<attribute name="OC_FARNELL" value="1838950"/>
<attribute name="OC_NEWARK" value="17M1783"/>
</technology>
<technology name="0048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP310048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3569"/>
</technology>
<technology name="0060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0110">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP310110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="97C5675"/>
</technology>
</technologies>
</device>
<device name="7" package="RT-C/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="OA" pad="12A"/>
<connect gate="2" pin="OB" pad="12B"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP710005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="52F964"/>
</technology>
<technology name="0006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP710006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3633"/>
</technology>
<technology name="0012">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="RP710012"/>
<attribute name="OC_FARNELL" value="388312"/>
<attribute name="OC_NEWARK" value="50H2650"/>
</technology>
<technology name="0024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP710024"/>
<attribute name="OC_FARNELL" value="388324"/>
<attribute name="OC_NEWARK" value="17M1785"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP710048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7825"/>
</technology>
<technology name="0060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?3*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S-X2"/>
</gates>
<devices>
<device name="3" package="RT-N/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP330048"/>
<attribute name="OC_FARNELL" value="388178"/>
<attribute name="OC_NEWARK" value="48M7779"/>
</technology>
</technologies>
</device>
<device name="7" package="RT-N/O16A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?31*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 / 12 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="4" package="RT-N/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="4-1393231-5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="13H3096"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="8" package="RT-N/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?32*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 / 12 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="4" package="RT-N/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP432024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3615"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="8" package="RT-N/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="2-1393232-4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="12H2332"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?12*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 / 12 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="8" package="RT-C/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP812024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3648"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="4" package="RT-C/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="1393231-8"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="11H3247"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP412012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3590"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP412024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7788"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP412110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7789"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?11*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 / 12 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="4" package="RT-C/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP411012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7784"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP411024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7785"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP411110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7786"/>
</technology>
</technologies>
</device>
<device name="8" package="RT-C/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP811024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7836"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?10*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 / 12 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="4" package="RT-C/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="8" package="RT-C/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP810012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7834"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="9-1393231-2"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H8837"/>
</technology>
<technology name="048">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP810048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3642"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?18*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 / 12 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="8" package="RT-C/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP818005"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7838"/>
</technology>
<technology name="006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP818006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3653"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP818012"/>
<attribute name="OC_FARNELL" value="388270"/>
<attribute name="OC_NEWARK" value="52F974"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP818024"/>
<attribute name="OC_FARNELL" value="388282"/>
<attribute name="OC_NEWARK" value="20C8802"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="4" package="RT-C/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP418006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7790"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP418012."/>
<attribute name="OC_FARNELL" value="388191"/>
<attribute name="OC_NEWARK" value="14J7708"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP418024"/>
<attribute name="OC_FARNELL" value="388221"/>
<attribute name="OC_NEWARK" value="17M1784"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP418048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7792"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP418110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7793"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?30*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 / 12 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="4" package="RT-N/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="8" package="RT-N/O12A5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?38*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/1&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 / 12 A&lt;br&gt;
Source: http://www.schrack.com/.. 5834.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="4" package="RT-N/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="9-1393232-3"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H8839"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP438024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3617"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="8" package="RT-N/O12A3.5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP838006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="52F982"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP838012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7858"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP838024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="52F984"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?SLF*" prefix="K">
<description>&lt;b&gt;Special Load PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A, for high inrush currents, bistable&lt;br&gt;
Source: http://www.schrack.com/.. 5837.pdf</description>
<gates>
<gate name="1" symbol="+KS+KR-"/>
<gate name="2" symbol="S-X2"/>
</gates>
<devices>
<device name="3" package="RP-SLF">
<connects>
<connect gate="1" pin="-" pad="A3"/>
<connect gate="1" pin="R+" pad="A1"/>
<connect gate="1" pin="S+" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP3SLF12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6258"/>
</technology>
<technology name="24">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP3SLF24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3556"/>
</technology>
</technologies>
</device>
<device name="7" package="RP-SLF">
<connects>
<connect gate="1" pin="-" pad="A3"/>
<connect gate="1" pin="R+" pad="A1"/>
<connect gate="1" pin="S+" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP?SLA*" prefix="K">
<description>&lt;b&gt;Special Load PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 16 A, for high inrush currents, monostable&lt;br&gt;
Source: http://www.schrack.com/.. 5837.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S-X2"/>
</gates>
<devices>
<device name="3" package="RP-SLA">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="05">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP3SLA05"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3553"/>
</technology>
<technology name="12">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP3SLA12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3554"/>
</technology>
<technology name="24">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP3SLA24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3555"/>
</technology>
</technologies>
</device>
<device name="7" package="RP-SLA">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="PA" pad="11A"/>
<connect gate="2" pin="PB" pad="11B"/>
<connect gate="2" pin="SA" pad="14A"/>
<connect gate="2" pin="SB" pad="14B"/>
</connects>
<technologies>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="6-1393231-4"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H0754"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT42?*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A, DC and AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5842.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="4" package="RT2C/O">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT424005"/>
<attribute name="OC_FARNELL" value="1629052"/>
<attribute name="OC_NEWARK" value="03P2425"/>
</technology>
<technology name="006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT424006"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3752"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT424012"/>
<attribute name="OC_FARNELL" value="1629053"/>
<attribute name="OC_NEWARK" value="03P2426"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT424024"/>
<attribute name="OC_FARNELL" value="1629054"/>
<attribute name="OC_NEWARK" value="16F393"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT424048"/>
<attribute name="OC_FARNELL" value="1629055"/>
<attribute name="OC_NEWARK" value="03P2428"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT424110"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="93B6583"/>
</technology>
<technology name="524">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT424524"/>
<attribute name="OC_FARNELL" value="1629056"/>
<attribute name="OC_NEWARK" value="94C4293"/>
</technology>
<technology name="615">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT424615"/>
<attribute name="OC_FARNELL" value="1629057"/>
<attribute name="OC_NEWARK" value="48F1292"/>
</technology>
<technology name="730">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT424730"/>
<attribute name="OC_FARNELL" value="1629058"/>
<attribute name="OC_NEWARK" value="85C0866"/>
</technology>
</technologies>
</device>
<device name="5" package="RT2C/O">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="22"/>
<connect gate="2" pin="P" pad="21"/>
<connect gate="2" pin="S" pad="24"/>
<connect gate="3" pin="O" pad="12"/>
<connect gate="3" pin="P" pad="11"/>
<connect gate="3" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="8-1393243-0"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H6457"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="8-1393243-2"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H6458"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="8-1393243-5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H6459"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="524">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT425524"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7992"/>
</technology>
<technology name="615">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT425615"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7993"/>
</technology>
<technology name="730">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="9-1393243-3"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="83H4419"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT44?*" prefix="K">
<description>&lt;b&gt;Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A, DC and AC-coil&lt;br&gt;
Source: http://www.schrack.com/.. 5842.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
</gates>
<devices>
<device name="4" package="RT2N/O">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="9-1393243-5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16H8852"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT444048"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7994"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="524">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT444524"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16R6383"/>
</technology>
<technology name="615">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RT444615"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="08H3757"/>
</technology>
<technology name="730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5" package="RT2N/O">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="524">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="615">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="730">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT424F*" prefix="K">
<description>&lt;b&gt;Power PCB Relay  polarized bistable version&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5843.pdf</description>
<gates>
<gate name="1" symbol="+KS+KR-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="4" package="RT424">
<connects>
<connect gate="1" pin="-" pad="A3"/>
<connect gate="1" pin="R+" pad="A2"/>
<connect gate="1" pin="S+" pad="A1"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RT424A*" prefix="K">
<description>&lt;b&gt;Power PCB Relay  polarized bistable version&lt;/b&gt; SCHRACK&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5843.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="" package="RT2C/O">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="O" pad="22"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="05">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT424A05"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7975"/>
</technology>
<technology name="06">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT424A06"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7976"/>
</technology>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT424A12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7977"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RT424A24"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7978"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP44?*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP II/2&lt;/b&gt; Schrack&lt;p&gt;
2 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 5844.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
<gate name="3" symbol="S"/>
</gates>
<devices>
<device name="" package="RP440">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="24"/>
</connects>
<technologies>
<technology name="0005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP440012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="07H9451"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP440024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7816"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="RP441012"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="09H1465"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP441024"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="48M7817"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP51*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP I&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A Vertical version&lt;br&gt;
Source: http://www.schrack.com/.. 5845.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="RP51">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP53*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP I&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A Vertical version&lt;br&gt;
Source: http://www.schrack.com/.. 5845.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="RP53">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0060">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RP530060-3-0"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="16C5685"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP61*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP I&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A Horizontal version&lt;br&gt;
Source: http://www.schrack.com/.. 5845.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="RP61">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="7060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RP63*" prefix="K">
<description>&lt;b&gt;Power PCB Relay RP I&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 8 A Horizontal version&lt;br&gt;
Source: http://www.schrack.com/.. 5845.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="RP63">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="0006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="0060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="1060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PB?14*" prefix="K">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1pole 10 A&lt;br&gt;
Source: http://www.schrack.com/.. 5846.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="1" package="PB">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="006">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="PB114006"/>
<attribute name="OC_FARNELL" value="1175076"/>
<attribute name="OC_NEWARK" value="85C1482"/>
</technology>
<technology name="012">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="PB114012"/>
<attribute name="OC_FARNELL" value="1175077"/>
<attribute name="OC_NEWARK" value="34K8593"/>
</technology>
<technology name="024">
<attribute name="MF" value="TYCO ELECTRONICS"/>
<attribute name="MPN" value="PB114024"/>
<attribute name="OC_FARNELL" value="1175078"/>
<attribute name="OC_NEWARK" value="34K8594"/>
</technology>
</technologies>
</device>
<device name="3" package="PB">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PB?34*" prefix="K">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1pole 10 A&lt;br&gt;
Source: http://www.schrack.com/.. 5846.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="3" package="PB">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="1" package="PB">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZNS1*" prefix="K">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1pole 10 A&lt;br&gt;
Source: http://www.schrack.com/.. 5847.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="ZN1">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="106">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="112">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="124">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="136">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="148">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="406">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="412">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="424">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="436">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="448">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZNS5*" prefix="K">
<description>&lt;b&gt;Miniature Power PCB Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1pole 10 A&lt;br&gt;
Source: http://www.schrack.com/.. 5847.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="ZN5">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="106">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="112">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="124">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="136">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="148">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="406">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="412">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="424">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="436">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="448">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZD?1*" prefix="K">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 30 A&lt;br&gt;
Source: http://www.schrack.com/.. 5848.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="3" package="ZD1">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5" package="ZD1F">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="12"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ZD?2*" prefix="K">
<description>&lt;b&gt;Power Relay&lt;/b&gt; SCHRACK&lt;p&gt;
1 pole 30 A&lt;br&gt;
Source: http://www.schrack.com/.. 5848.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="3" package="ZD2">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="5" package="ZD2F">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="P" pad="11"/>
<connect gate="2" pin="S" pad="14"/>
</connects>
<technologies>
<technology name="2006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRD4*" prefix="K">
<description>&lt;b&gt;Safety Relay&lt;/b&gt; SCHRACK&lt;p&gt;
4 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 6685.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="O"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="S"/>
</gates>
<devices>
<device name="" package="SR4">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="12"/>
<connect gate="3" pin="O" pad="21"/>
<connect gate="3" pin="P" pad="22"/>
<connect gate="4" pin="P" pad="34"/>
<connect gate="4" pin="S" pad="33"/>
<connect gate="5" pin="P" pad="44"/>
<connect gate="5" pin="S" pad="43"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="015">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="018">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="021">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="036">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="040">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="085">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SRM4*" prefix="K">
<description>&lt;b&gt;Safety Relay&lt;/b&gt; SCHRACK&lt;p&gt;
4 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 6685.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="S"/>
</gates>
<devices>
<device name="" package="SR4">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="12"/>
<connect gate="3" pin="P" pad="21"/>
<connect gate="3" pin="S" pad="22"/>
<connect gate="4" pin="P" pad="34"/>
<connect gate="4" pin="S" pad="33"/>
<connect gate="5" pin="P" pad="44"/>
<connect gate="5" pin="S" pad="43"/>
</connects>
<technologies>
<technology name="005">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="006">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="009">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="012">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="015">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="018">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="021">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="024">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="036">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="040">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="048">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="060">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="085">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SR6B4*" prefix="K">
<description>&lt;b&gt;Safety Relay SR6&lt;/b&gt; SCHRACK&lt;p&gt;
sensitive 6 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 6688.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="O"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="S"/>
<gate name="6" symbol="S"/>
<gate name="7" symbol="S"/>
</gates>
<devices>
<device name="" package="SR6B">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="12"/>
<connect gate="3" pin="O" pad="21"/>
<connect gate="3" pin="P" pad="22"/>
<connect gate="4" pin="P" pad="34"/>
<connect gate="4" pin="S" pad="33"/>
<connect gate="5" pin="P" pad="44"/>
<connect gate="5" pin="S" pad="43"/>
<connect gate="6" pin="P" pad="54"/>
<connect gate="6" pin="S" pad="53"/>
<connect gate="7" pin="P" pad="64"/>
<connect gate="7" pin="S" pad="63"/>
</connects>
<technologies>
<technology name="S05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S18">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S21">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S36">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S40">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SR6A4*" prefix="K">
<description>&lt;b&gt;Safety Relay SR6&lt;/b&gt; SCHRACK&lt;p&gt;
sensitive 6 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 6688.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="O"/>
<gate name="4" symbol="O"/>
<gate name="5" symbol="S"/>
<gate name="6" symbol="S"/>
<gate name="7" symbol="S"/>
</gates>
<devices>
<device name="" package="SR6A">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="12"/>
<connect gate="3" pin="O" pad="21"/>
<connect gate="3" pin="P" pad="22"/>
<connect gate="4" pin="O" pad="31"/>
<connect gate="4" pin="P" pad="32"/>
<connect gate="5" pin="P" pad="44"/>
<connect gate="5" pin="S" pad="43"/>
<connect gate="6" pin="P" pad="54"/>
<connect gate="6" pin="S" pad="53"/>
<connect gate="7" pin="P" pad="64"/>
<connect gate="7" pin="S" pad="63"/>
</connects>
<technologies>
<technology name="S05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S18">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S21">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S36">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S40">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SR6C4*" prefix="K">
<description>&lt;b&gt;Safety Relay SR6&lt;/b&gt; SCHRACK&lt;p&gt;
sensitive 6 pole 8 A&lt;br&gt;
Source: http://www.schrack.com/.. 6688.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="O"/>
<gate name="3" symbol="S"/>
<gate name="4" symbol="S"/>
<gate name="5" symbol="S"/>
<gate name="6" symbol="S"/>
<gate name="7" symbol="S"/>
</gates>
<devices>
<device name="" package="SR6C">
<connects>
<connect gate="1" pin="1" pad="A1"/>
<connect gate="1" pin="2" pad="A2"/>
<connect gate="2" pin="O" pad="21"/>
<connect gate="2" pin="P" pad="22"/>
<connect gate="3" pin="P" pad="14"/>
<connect gate="3" pin="S" pad="13"/>
<connect gate="4" pin="P" pad="34"/>
<connect gate="4" pin="S" pad="33"/>
<connect gate="5" pin="P" pad="44"/>
<connect gate="5" pin="S" pad="43"/>
<connect gate="6" pin="P" pad="54"/>
<connect gate="6" pin="S" pad="53"/>
<connect gate="7" pin="P" pad="64"/>
<connect gate="7" pin="S" pad="63"/>
</connects>
<technologies>
<technology name="S05">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S06">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S09">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S15">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S18">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S21">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S36">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S40">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="S48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NV2R" prefix="K">
<description>&lt;b&gt;MOTORUMPOL RELAIS 12V&lt;/b&gt;&lt;p&gt;
Ningbo Forward Relay Corporation LTD.&lt;br&gt;
Ningbo.Huaguan Electronics Corporation LTD.&lt;p&gt;
Source: http://www.dblectro.com/site/pdf/NV2R.pdf&lt;p&gt;
http://www2.produktinfo.conrad.com/datenblaetter/500000-524999/505013-da-01-de-Motorumpolrelais_12V.pdf&lt;br&gt;
Elli-Echo ER20T-S-DC12V - 20A/14VDC&lt;br&gt;
Conrad Nr.: 505013 - 62</description>
<gates>
<gate name="G$1" symbol="NV2R"/>
</gates>
<devices>
<device name="" package="NV2R">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="A+" pad="A+"/>
<connect gate="G$1" pin="A-" pad="A-"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="B+" pad="B+"/>
<connect gate="G$1" pin="B-" pad="B-"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6D?*" prefix="K">
<description>&lt;b&gt;OMRON Slim, Miniature PCB Relay&lt;/b&gt; 17.5 × 6.5 × 12.5 mm&lt;p&gt;
with Socked&lt;br&gt;
Source: http://ecb.omron.com.sg/pdf/relay/power/G6D.pdf</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="-1A-ASI" package="G6D">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="13"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="12VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5VDC">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="9812660"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="-04P" package="G6D-SOCKET">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="13"/>
<connect gate="2" pin="P" pad="7"/>
<connect gate="2" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G5SB" prefix="K">
<description>&lt;b&gt;Compact Single-pole Relay for Switching 5 A&lt;/b&gt;&lt;p&gt;
Source: http://www.omron.com/ecb/products/pry/121/g5sb.html</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="U" symbol="U"/>
</gates>
<devices>
<device name="" package="G5SB">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="5"/>
<connect gate="U" pin="O" pad="4"/>
<connect gate="U" pin="P" pad="2"/>
<connect gate="U" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="S*02S02" prefix="K">
<description>&lt;b&gt;IT(rms) 8A, Zero Cross type SIP 4pin Triac output SSR&lt;/b&gt;&lt;p&gt;
Source: http://sharp-world.com/products/device/lineup/data/pdf/datasheet/s102s02_e.pdf</description>
<gates>
<gate name="G$1" symbol="PHOTOTRIAC-Z"/>
</gates>
<devices>
<device name="" package="S202S02">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="2"/>
<connect gate="G$1" pin="K" pad="4"/>
</connects>
<technologies>
<technology name="1">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="2">
<attribute name="MF" value=""/>
<attribute name="MPN" value="S202S02F"/>
<attribute name="OC_FARNELL" value="1618475"/>
<attribute name="OC_NEWARK" value="14N9588"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G6J*-2?-Y" prefix="K">
<description>&lt;b&gt;Surface-Mounting Signal Relay - G6J-Y&lt;/b&gt; 5.7 x 10.6 x 9 mm&lt;p&gt;
Source: http://www.omroncomponents.eu/ .. K125-E2-02-X.pdf</description>
<gates>
<gate name="1" symbol="K+-"/>
<gate name="2" symbol="U"/>
<gate name="3" symbol="U"/>
</gates>
<devices>
<device name="P" package="G6J-2P-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6J-2P-Y-DC12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70J9830"/>
</technology>
<technology name="U">
<attribute name="MF" value="OMRON COMPONENTS USA"/>
<attribute name="MPN" value="G6JU-2P-Y-DC12"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70J9842"/>
</technology>
</technologies>
</device>
<device name="FS" package="G6J-2FS-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="G6J-2FS-Y DC4.5"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="04M9910"/>
</technology>
<technology name="U">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="FL" package="G6J-2FL-Y">
<connects>
<connect gate="1" pin="+" pad="1"/>
<connect gate="1" pin="-" pad="8"/>
<connect gate="2" pin="O" pad="2"/>
<connect gate="2" pin="P" pad="3"/>
<connect gate="2" pin="S" pad="4"/>
<connect gate="3" pin="O" pad="7"/>
<connect gate="3" pin="P" pad="6"/>
<connect gate="3" pin="S" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="G6J-2FL-Y-TR DC4.5"/>
<attribute name="OC_FARNELL" value="1798618"/>
<attribute name="OC_NEWARK" value="04M9907"/>
</technology>
<technology name="U">
<attribute name="MF" value=""/>
<attribute name="MPN" value="G6JU-2FL-Y DC3"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="04M9916"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="G5V-2" prefix="K">
<description>&lt;b&gt;OMRON PCB Relay&lt;/b&gt;&lt;p&gt;
Source: http://www.omron.com/ecb/products/pdf/en-g5v2.pdf</description>
<gates>
<gate name="A" symbol="K"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="G5V-2">
<connects>
<connect gate="1" pin="O" pad="6"/>
<connect gate="1" pin="P" pad="4"/>
<connect gate="1" pin="S" pad="8"/>
<connect gate="2" pin="O" pad="11"/>
<connect gate="2" pin="P" pad="13"/>
<connect gate="2" pin="S" pad="9"/>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="16"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="G5V-2 5DC"/>
<attribute name="OC_FARNELL" value="9949488"/>
<attribute name="OC_NEWARK" value="78K5703"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BT-*-S" prefix="K">
<description>&lt;b&gt;KLEIN RELAIS WASCHDICHT&lt;/b&gt; 2 Wechsler&lt;p&gt;
Distriibutor: Conrad Electronic, Bestell Nr.:&lt;br&gt;
505226-13 - 24V&lt;br&gt;
505226-13 - 5V&lt;br&gt;
505170-13 - 12V&lt;br&gt;
505170-13 - 48V&lt;br&gt;
Bestar Electric Ltd.&lt;/br&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/500000-524999/505226-da-01-en-Kleinrelais_waschdicht_24V.pdf</description>
<gates>
<gate name="K" symbol="K"/>
<gate name="-1" symbol="U"/>
<gate name="-2" symbol="U"/>
</gates>
<devices>
<device name="" package="BT-XX-S">
<connects>
<connect gate="-1" pin="O" pad="6"/>
<connect gate="-1" pin="P" pad="4"/>
<connect gate="-1" pin="S" pad="8"/>
<connect gate="-2" pin="O" pad="11"/>
<connect gate="-2" pin="P" pad="13"/>
<connect gate="-2" pin="S" pad="9"/>
<connect gate="K" pin="1" pad="1"/>
<connect gate="K" pin="2" pad="16"/>
</connects>
<technologies>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="9">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTR-K1C" prefix="K">
<description>&lt;b&gt;NETZRELAIS FTR-K1CK024W1XUM 16A/250VAC&lt;/b&gt; 1 Umschaltkontakt&lt;p&gt;
Distributor: Conrad Electronic&lt;br&gt;
Bestell Nr.:&lt;br&gt;
504389-13 - 24V&lt;br&gt;
Source: http://www.produktinfo.conrad.com/datenblaetter/500000-524999/504384-da-01-de-NETZRELAIS_FTR_K1CK012W1XUM_16A_250VAC.pdf</description>
<gates>
<gate name="K" symbol="K"/>
<gate name="-1" symbol="U-X2"/>
</gates>
<devices>
<device name="" package="FTR-K1C">
<connects>
<connect gate="-1" pin="OA" pad="2"/>
<connect gate="-1" pin="OB" pad="7"/>
<connect gate="-1" pin="PA" pad="3"/>
<connect gate="-1" pin="PB" pad="6"/>
<connect gate="-1" pin="SA" pad="4"/>
<connect gate="-1" pin="SB" pad="5"/>
<connect gate="K" pin="1" pad="1"/>
<connect gate="K" pin="2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTR-LYC" prefix="K">
<description>&lt;b&gt;Schmales Netzrelais&lt;/b&gt;&lt;p&gt;
NETZRELAIS FTR-LYCA024V 1XUM 6A/250VAC&lt;br&gt;
Distributor: Conrad electronic&lt;br&gt;
Bestell Nr.: 504382 - 62 &lt;br&gt;
Source: http://www2.produktinfo.conrad.com/datenblaetter/500000-524999/504382-da-01-de-NETZRELAIS_FTR-LYCA024V_1XUM_6A_250VAC.pdf</description>
<gates>
<gate name="K" symbol="K"/>
<gate name="-1" symbol="U"/>
</gates>
<devices>
<device name="" package="FTR-LYC">
<connects>
<connect gate="-1" pin="O" pad="3"/>
<connect gate="-1" pin="P" pad="4"/>
<connect gate="-1" pin="S" pad="5"/>
<connect gate="K" pin="1" pad="1"/>
<connect gate="K" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="5">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="6">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FINDER-30.22" prefix="K">
<description>&lt;b&gt;SUBMINIATURE DIL-RELAIS&lt;/b&gt; FINDER 30.22.9.024.0000&lt;p&gt;
Kontakt max. AC - 125V&lt;br&gt;
Distributor: Farnell&lt;br&gt;
Bestell Nr.: 1217371&lt;br&gt;
Source: http://www.farnell.com/datasheets/87634.pdf</description>
<gates>
<gate name="K" symbol="K"/>
<gate name="-1" symbol="U"/>
<gate name="-2" symbol="U"/>
</gates>
<devices>
<device name="" package="FINDER-30.22">
<connects>
<connect gate="-1" pin="O" pad="12"/>
<connect gate="-1" pin="P" pad="11"/>
<connect gate="-1" pin="S" pad="14"/>
<connect gate="-2" pin="O" pad="22"/>
<connect gate="-2" pin="P" pad="21"/>
<connect gate="-2" pin="S" pad="24"/>
<connect gate="K" pin="1" pad="A1"/>
<connect gate="K" pin="2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FINDER-43.61" prefix="K">
<description>&lt;b&gt;Low profile PCB relays 10 - 16 A&lt;/b&gt; FINDER 43 Series&lt;p&gt;
Kontakt max. AC- 250V,  Strom - Kontakt  AC- max. 10A&lt;br&gt;
5 mm contact pin pitch,  1 Pole NO, 16 A, PCB mount&lt;br&gt;
Distributor: FARNELL&lt;br&gt;
Source: http://www.farnell.com/datasheets/87682.pdf</description>
<gates>
<gate name="K" symbol="K"/>
<gate name="-1" symbol="S-X2"/>
</gates>
<devices>
<device name="" package="FINDER-43.61">
<connects>
<connect gate="-1" pin="PA" pad="11@1"/>
<connect gate="-1" pin="PB" pad="11@2"/>
<connect gate="-1" pin="SA" pad="14@1"/>
<connect gate="-1" pin="SB" pad="14@2"/>
<connect gate="K" pin="1" pad="A1"/>
<connect gate="K" pin="2" pad="A2"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AZ8-FORM-C" prefix="K">
<description>&lt;b&gt;MINIATURE PC BOARD RELAY&lt;/b&gt; Form C&lt;p&gt;
Source: www.azettler.com .. AZ8-1ch-12DSE.PDF</description>
<gates>
<gate name="K" symbol="K"/>
<gate name="-1" symbol="U"/>
</gates>
<devices>
<device name="" package="AZ8">
<connects>
<connect gate="-1" pin="O" pad="4"/>
<connect gate="-1" pin="P" pad="1"/>
<connect gate="-1" pin="S" pad="3"/>
<connect gate="K" pin="1" pad="2"/>
<connect gate="K" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AZ8-FORM-A" prefix="K">
<description>&lt;b&gt;MINIATURE PC BOARD RELAY&lt;/b&gt; Form A&lt;p&gt;
Source: www.azettler.com .. AZ8-1ch-12DSE.PDF</description>
<gates>
<gate name="K" symbol="K"/>
<gate name="-1" symbol="S"/>
</gates>
<devices>
<device name="" package="AZ8">
<connects>
<connect gate="-1" pin="P" pad="1"/>
<connect gate="-1" pin="S" pad="3"/>
<connect gate="K" pin="1" pad="2"/>
<connect gate="K" pin="2" pad="5"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="9802" prefix="K">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt;&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
<gates>
<gate name="P" symbol="9802"/>
</gates>
<devices>
<device name="-00" package="9802-00">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
<connect gate="P" pin="3" pad="3"/>
<connect gate="P" pin="4" pad="4"/>
<connect gate="P" pin="5" pad="5"/>
<connect gate="P" pin="6" pad="6"/>
<connect gate="P" pin="7" pad="7"/>
<connect gate="P" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="-03">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-05">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9802-05-00"/>
<attribute name="OC_FARNELL" value="1081689"/>
<attribute name="OC_NEWARK" value="16F3689"/>
</technology>
</technologies>
</device>
<device name="-20" package="9802-20">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
<connect gate="P" pin="3" pad="3"/>
<connect gate="P" pin="4" pad="4"/>
<connect gate="P" pin="5" pad="5"/>
<connect gate="P" pin="6" pad="6"/>
<connect gate="P" pin="7" pad="7"/>
<connect gate="P" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="-03">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="-05">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9802-05-20"/>
<attribute name="OC_FARNELL" value="1081633"/>
<attribute name="OC_NEWARK" value="92F3367"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="9814" prefix="K">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt;&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
<gates>
<gate name="P" symbol="9802"/>
</gates>
<devices>
<device name="-00" package="9814-00">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
<connect gate="P" pin="3" pad="3"/>
<connect gate="P" pin="4" pad="4"/>
<connect gate="P" pin="5" pad="5"/>
<connect gate="P" pin="6" pad="6"/>
<connect gate="P" pin="7" pad="7"/>
<connect gate="P" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="-03">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9814-03-00"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="29H2537"/>
</technology>
<technology name="-05">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9814-05-00"/>
<attribute name="OC_FARNELL" value="1081691"/>
<attribute name="OC_NEWARK" value="29H2538"/>
</technology>
</technologies>
</device>
<device name="-20" package="9814-20">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
<connect gate="P" pin="3" pad="3"/>
<connect gate="P" pin="4" pad="4"/>
<connect gate="P" pin="5" pad="5"/>
<connect gate="P" pin="6" pad="6"/>
<connect gate="P" pin="7" pad="7"/>
<connect gate="P" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="-03">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9814-03-20"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="83H2026"/>
</technology>
<technology name="-05">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9814-05-20"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="83H2028"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="9852" prefix="K">
<description>&lt;b&gt;Surface Mount Reed Relays&lt;/b&gt;&lt;p&gt;
Source: COTO TECHNOLOGY - 9852-03-00 - RELAY - 91349.pdf</description>
<gates>
<gate name="P" symbol="9852"/>
</gates>
<devices>
<device name="-00" package="9852-00">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
<connect gate="P" pin="3" pad="3"/>
<connect gate="P" pin="4" pad="4"/>
<connect gate="P" pin="5" pad="5"/>
<connect gate="P" pin="6" pad="6"/>
<connect gate="P" pin="7" pad="7"/>
<connect gate="P" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="-03">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9852-03-00"/>
<attribute name="OC_FARNELL" value="1081692"/>
<attribute name="OC_NEWARK" value="29H2540"/>
</technology>
<technology name="-05">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9852-05-00"/>
<attribute name="OC_FARNELL" value="1081693"/>
<attribute name="OC_NEWARK" value="84C8955"/>
</technology>
</technologies>
</device>
<device name="-20" package="9852-20">
<connects>
<connect gate="P" pin="1" pad="1"/>
<connect gate="P" pin="2" pad="2"/>
<connect gate="P" pin="3" pad="3"/>
<connect gate="P" pin="4" pad="4"/>
<connect gate="P" pin="5" pad="5"/>
<connect gate="P" pin="6" pad="6"/>
<connect gate="P" pin="7" pad="7"/>
<connect gate="P" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="-03">
<attribute name="MF" value="COTO TECHNOLOGY"/>
<attribute name="MPN" value="9852-03-20"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="83H2030"/>
</technology>
<technology name="-05">
<attribute name="MF" value=""/>
<attribute name="MPN" value="9852-05-20"/>
<attribute name="OC_FARNELL" value="1081642"/>
<attribute name="OC_NEWARK" value="46M4523"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="6561-0300" prefix="K">
<description>&lt;b&gt;20 / 30 A-Leistungsrelais&lt;/b&gt;&lt;p&gt;
Source: http://www.finder.de/comuni/pdf/S65DE.pdf</description>
<gates>
<gate name="1" symbol="K-2P"/>
<gate name="2" symbol="S-2P"/>
<gate name="-1" symbol="O-2P"/>
</gates>
<devices>
<device name="" package="6561-0300">
<connects>
<connect gate="-1" pin="O" pad="14"/>
<connect gate="-1" pin="O_" pad="14_"/>
<connect gate="-1" pin="P" pad="22"/>
<connect gate="-1" pin="P_" pad="22_"/>
<connect gate="1" pin="1" pad="A1_"/>
<connect gate="1" pin="1_" pad="A1"/>
<connect gate="1" pin="2" pad="A2_"/>
<connect gate="1" pin="2_" pad="A2"/>
<connect gate="2" pin="P" pad="11_"/>
<connect gate="2" pin="P_" pad="11"/>
<connect gate="2" pin="S" pad="21_"/>
<connect gate="2" pin="S_" pad="21"/>
</connects>
<technologies>
<technology name="VAC110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC120">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC230">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC240">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC400">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC6">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VAC60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VDC110">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VDC12">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VDC125">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VDC220">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VDC24">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VDC48">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VDC6">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
<technology name="VDC60">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQW27" prefix="K">
<description>&lt;b&gt;PhotoMOSS RELAYS&lt;/b&gt; PD Type 2- channel (Form a) Type&lt;p&gt;
Source: http://www.ic-on-line.cn/IOL/datasheet/aqw277az_1212830.pdf</description>
<gates>
<gate name="A" symbol="PHOTO-RELAY-2S"/>
<gate name="B" symbol="PHOTO-RELAY-2S"/>
</gates>
<devices>
<device name="" package="AQW27-DIL08">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="D1" pad="8"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="K" pad="2"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="D1" pad="6"/>
<connect gate="B" pin="D2" pad="5"/>
<connect gate="B" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="A" package="AQW27-SMD08">
<connects>
<connect gate="A" pin="A" pad="1"/>
<connect gate="A" pin="D1" pad="8"/>
<connect gate="A" pin="D2" pad="7"/>
<connect gate="A" pin="K" pad="2"/>
<connect gate="B" pin="A" pad="3"/>
<connect gate="B" pin="D1" pad="6"/>
<connect gate="B" pin="D2" pad="5"/>
<connect gate="B" pin="K" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="AQZ26" prefix="K">
<description>&lt;b&gt;PhotoMOS Relays Power 1 Form A&lt;/b&gt; High capacity up to 6A in a slim SIL package&lt;p&gt;
Source: http://www.panasonic-electric-works.com/catalogues/downloads/photomos/ds_x615_en_aqz262_264.pdf</description>
<gates>
<gate name="A" symbol="PHOTOMOS_2D"/>
</gates>
<devices>
<device name="" package="AQZ26-SIL04">
<connects>
<connect gate="A" pin="A" pad="2"/>
<connect gate="A" pin="DS1" pad="3"/>
<connect gate="A" pin="DS2" pad="4"/>
<connect gate="A" pin="K" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CPC1708J" prefix="K">
<description>&lt;b&gt;Single-Pole, Normally Open i4-PAC (TM)&lt;/b&gt; DC Power Relay&lt;p&gt;
Source: &lt;a href="http://www.clare.com/home/pdfs.nsf/www/CPC1708.pdf/$file/CPC1708.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="PHOTOMOS_DC"/>
</gates>
<devices>
<device name="" package="I4-PAC">
<connects>
<connect gate="G$1" pin="A" pad="4"/>
<connect gate="G$1" pin="DS1" pad="1"/>
<connect gate="G$1" pin="DS2" pad="2"/>
<connect gate="G$1" pin="K" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FTR-B4" prefix="K">
<description>&lt;b&gt;ULTRA MINIATURE RELAY 2 POLES - 2 A&lt;/b&gt; (Slim Profile Signal Relay)&lt;p&gt;
FUJITSU FTR-B4 SERIES&lt;br&gt;
Source: FTR-B4.pdf</description>
<gates>
<gate name="K" symbol="K+-"/>
<gate name="-1" symbol="U"/>
<gate name="-2" symbol="U"/>
</gates>
<devices>
<device name="C" package="FTR-B4C">
<connects>
<connect gate="-1" pin="O" pad="2"/>
<connect gate="-1" pin="P" pad="3"/>
<connect gate="-1" pin="S" pad="4"/>
<connect gate="-2" pin="O" pad="7"/>
<connect gate="-2" pin="P" pad="6"/>
<connect gate="-2" pin="S" pad="5"/>
<connect gate="K" pin="+" pad="1"/>
<connect gate="K" pin="-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="G" package="FTR-B4G">
<connects>
<connect gate="-1" pin="O" pad="2"/>
<connect gate="-1" pin="P" pad="3"/>
<connect gate="-1" pin="S" pad="4"/>
<connect gate="-2" pin="O" pad="7"/>
<connect gate="-2" pin="P" pad="6"/>
<connect gate="-2" pin="S" pad="5"/>
<connect gate="K" pin="+" pad="1"/>
<connect gate="K" pin="-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="FTR-B4S">
<connects>
<connect gate="-1" pin="O" pad="2"/>
<connect gate="-1" pin="P" pad="3"/>
<connect gate="-1" pin="S" pad="4"/>
<connect gate="-2" pin="O" pad="7"/>
<connect gate="-2" pin="P" pad="6"/>
<connect gate="-2" pin="S" pad="5"/>
<connect gate="K" pin="+" pad="1"/>
<connect gate="K" pin="-" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JW1A" prefix="K">
<description>&lt;b&gt;Power relay&lt;/b&gt;&lt;p&gt;
Source: Panasonic Electric Works Co., Ltd. / jw.catalog.pdf</description>
<gates>
<gate name="_" symbol="K"/>
<gate name="1" symbol="S"/>
</gates>
<devices>
<device name="" package="JW1A">
<connects>
<connect gate="1" pin="P" pad="6"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JW1C" prefix="K">
<description>&lt;b&gt;Power relay&lt;/b&gt;&lt;p&gt;
Source: Panasonic Electric Works Co., Ltd. / jw.catalog.pdf</description>
<gates>
<gate name="_" symbol="K"/>
<gate name="1" symbol="U"/>
</gates>
<devices>
<device name="" package="JW1C">
<connects>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="6"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JW2A" prefix="K">
<description>&lt;b&gt;Power relay&lt;/b&gt;&lt;p&gt;
Source: Panasonic Electric Works Co., Ltd. / jw.catalog.pdf</description>
<gates>
<gate name="_" symbol="K"/>
<gate name="1" symbol="S"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="JW2A">
<connects>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="P" pad="6"/>
<connect gate="2" pin="S" pad="5"/>
<connect gate="_" pin="1" pad="1"/>
<connect gate="_" pin="2" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JW2C" prefix="K">
<description>&lt;b&gt;Power relay&lt;/b&gt;&lt;p&gt;
Source: Panasonic Electric Works Co., Ltd. / jw.catalog.pdf</description>
<gates>
<gate name="-" symbol="K"/>
<gate name="1" symbol="U"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="JW2C">
<connects>
<connect gate="-" pin="1" pad="1"/>
<connect gate="-" pin="2" pad="8"/>
<connect gate="1" pin="O" pad="2"/>
<connect gate="1" pin="P" pad="3"/>
<connect gate="1" pin="S" pad="4"/>
<connect gate="2" pin="O" pad="7"/>
<connect gate="2" pin="P" pad="6"/>
<connect gate="2" pin="S" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JV*-KT" prefix="K">
<description>&lt;b&gt;POWER RELAY JV SERIES&lt;/b&gt; 1 POLE—5 A (MEDIUM LOAD CONTROL) &lt;p&gt;
Source: &lt;a href="http://www.produktinfo.conrad.com/datenblaetter/500000-524999/502946-da-01-en-RELAIS_JV_12S_KT.pdf"&gt; Data sheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="K"/>
<gate name="G$2" symbol="S"/>
</gates>
<devices>
<device name="" package="JV-KT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$2" pin="P" pad="2"/>
<connect gate="G$2" pin="S" pad="3"/>
</connects>
<technologies>
<technology name="-12"/>
<technology name="-12S"/>
<technology name="-18S"/>
<technology name="-24"/>
<technology name="-24S"/>
<technology name="-3"/>
<technology name="-3S"/>
<technology name="-48"/>
<technology name="-5"/>
<technology name="-5S"/>
<technology name="-6"/>
<technology name="-6S"/>
<technology name="-9"/>
<technology name="-9S"/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="APF30212A" prefix="K">
<description>&lt;b&gt;Compliant with European standards 1a/1c 6A Slim power relays&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://pewa.panasonic.com/assets/pcsd/catalog/pf-catalog.pdf"&gt;Data sheet &lt;/a&gt;</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="S"/>
</gates>
<devices>
<device name="" package="APF30212A">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="APF30212C" prefix="K">
<description>&lt;b&gt;Compliant with European standards 1a/1c 6A Slim power relays&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://pewa.panasonic.com/assets/pcsd/catalog/pf-catalog.pdf"&gt;Data sheet &lt;/a&gt;</description>
<gates>
<gate name="1" symbol="K"/>
<gate name="2" symbol="U"/>
</gates>
<devices>
<device name="" package="APF30212C">
<connects>
<connect gate="1" pin="1" pad="1"/>
<connect gate="1" pin="2" pad="2"/>
<connect gate="2" pin="O" pad="NC"/>
<connect gate="2" pin="P" pad="COM"/>
<connect gate="2" pin="S" pad="NO"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
