<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<library>
<description>&lt;b&gt;R. F. Solutions Ltd.&lt;/b&gt;&lt;p&gt;
R F Solutions is a member of the Low Power Radio Association.&lt;br&gt;
http://www.rfsolutions.co.uk&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-18W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="SO-08">
<description>&lt;B&gt;Small Outline Narrow Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
150-mil body, package type SN</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="DIL18">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="RF600E">
<pin name="S0" direction="in"/>
<pin name="S1" direction="in"/>
<pin name="S2" direction="in"/>
<pin name="S3" direction="in"/>
<pin name="LED" direction="out"/>
<pin name="DO" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
<symbol name="RF600D">
<pin name="LKIN" direction="in"/>
<pin name="LRN" direction="in"/>
<pin name="IN" direction="in"/>
<pin name="ECLK" direction="out"/>
<pin name="SD1" direction="out"/>
<pin name="LB" direction="out"/>
<pin name="OP1" direction="out"/>
<pin name="OP2" direction="out"/>
<pin name="OP3" direction="out"/>
<pin name="OP4" direction="out"/>
<pin name="SLEEP" direction="in"/>
<pin name="VCC@1" direction="pwr"/>
<pin name="VCC" direction="in"/>
<pin name="GND" direction="pwr"/>
<pin name="EDAT"/>
<pin name="ECS" direction="out"/>
</symbol>
<symbol name="RF600D8">
<pin name="IN" direction="in"/>
<pin name="SD" direction="out"/>
<pin name="MS" direction="out"/>
<pin name="VCC" direction="pwr"/>
<pin name="GND" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RF600D" prefix="IC">
<description>&lt;b&gt;RF / IR Decoder&lt;/b&gt;&lt;p&gt;
Source: RF600D.pdf</description>
<gates>
<gate name="G$1" symbol="RF600D"/>
</gates>
<devices>
<device name="-SO" package="SO-18W">
<connects>
<connect gate="G$1" pin="ECLK" pad="7"/>
<connect gate="G$1" pin="ECS" pad="6"/>
<connect gate="G$1" pin="EDAT" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN" pad="9"/>
<connect gate="G$1" pin="LB" pad="3"/>
<connect gate="G$1" pin="LKIN" pad="12"/>
<connect gate="G$1" pin="LRN" pad="10"/>
<connect gate="G$1" pin="OP1" pad="17"/>
<connect gate="G$1" pin="OP2" pad="18"/>
<connect gate="G$1" pin="OP3" pad="1"/>
<connect gate="G$1" pin="OP4" pad="2"/>
<connect gate="G$1" pin="SD1" pad="11"/>
<connect gate="G$1" pin="SLEEP" pad="13"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="RF600D-SO"/>
<attribute name="OC_FARNELL" value="8733813"/>
<attribute name="OC_NEWARK" value="18K6846"/>
</technology>
</technologies>
</device>
<device name="" package="DIL18">
<connects>
<connect gate="G$1" pin="ECLK" pad="7"/>
<connect gate="G$1" pin="ECS" pad="6"/>
<connect gate="G$1" pin="EDAT" pad="8"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="IN" pad="9"/>
<connect gate="G$1" pin="LB" pad="3"/>
<connect gate="G$1" pin="LKIN" pad="12"/>
<connect gate="G$1" pin="LRN" pad="10"/>
<connect gate="G$1" pin="OP1" pad="17"/>
<connect gate="G$1" pin="OP2" pad="18"/>
<connect gate="G$1" pin="OP3" pad="1"/>
<connect gate="G$1" pin="OP4" pad="2"/>
<connect gate="G$1" pin="SD1" pad="11"/>
<connect gate="G$1" pin="SLEEP" pad="13"/>
<connect gate="G$1" pin="VCC" pad="4"/>
<connect gate="G$1" pin="VCC@1" pad="14"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RF600D"/>
<attribute name="OC_FARNELL" value="1200973"/>
<attribute name="OC_NEWARK" value="01M8597"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF600E" prefix="IC">
<description>&lt;b&gt;RF / IR Encoder&lt;/b&gt;&lt;p&gt;
Source: RF600D.pdf</description>
<gates>
<gate name="G$1" symbol="RF600E"/>
</gates>
<devices>
<device name="-SO" package="SO-08">
<connects>
<connect gate="G$1" pin="DO" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LED" pad="7"/>
<connect gate="G$1" pin="S0" pad="1"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="3"/>
<connect gate="G$1" pin="S3" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="RF600E-SO"/>
<attribute name="OC_FARNELL" value="8733805"/>
<attribute name="OC_NEWARK" value="18K6847"/>
</technology>
</technologies>
</device>
<device name="" package="DIL08">
<connects>
<connect gate="G$1" pin="DO" pad="6"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="LED" pad="7"/>
<connect gate="G$1" pin="S0" pad="1"/>
<connect gate="G$1" pin="S1" pad="2"/>
<connect gate="G$1" pin="S2" pad="3"/>
<connect gate="G$1" pin="S3" pad="4"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="RF600E"/>
<attribute name="OC_FARNELL" value="1200972"/>
<attribute name="OC_NEWARK" value="01M8598"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RF600?8" prefix="IC">
<description>&lt;b&gt;RF / IR Decoder&lt;/b&gt;&lt;p&gt;
Miniature 8 pin version option providing a serial data output only.&lt;br&gt;
Source: RF600D.pdf</description>
<gates>
<gate name="G$1" symbol="RF600D8"/>
</gates>
<devices>
<device name="DP" package="DIL08">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="MS" pad="6"/>
<connect gate="G$1" pin="SD" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
<device name="DS" package="SO-08">
<connects>
<connect gate="G$1" pin="GND" pad="8"/>
<connect gate="G$1" pin="IN" pad="4"/>
<connect gate="G$1" pin="MS" pad="6"/>
<connect gate="G$1" pin="SD" pad="2"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
