<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.2">
<drawing>
<library>
<description>&lt;b&gt;&lt;i&gt;Eurocircuits test-mate&lt;/i&gt; foot prints&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
This library contains the foot prints to be placed on the PCB to be tested.&lt;br&gt;
Version 1.0&lt;p&gt;

&lt;b&gt;&lt;i&gt;eC-test-mate&lt;/i&gt;&lt;/b&gt; is a handheld test system for functional testing of assembled PCBs without the need for complex tooling. Simply integrate eC-test-mate footprints into your PCB-layout, write your test programs, place the eC-test-mate test head(s) on your board and run the tests. No connectors, no test jigs, just easy footprints. eC-test-mate is a cost-effective solution for testing small series of assembled PCBs.&lt;p&gt;

More information on &lt;a href="http://www.eurocircuits.com/test"&gt;http://www.eurocircuits.com/test&lt;/a&gt;&lt;br&gt;&lt;p&gt;

&lt;img alt=EcTestMate src=http://www.eurocircuits.com/clientmedia/silderImages/picture1.png?v=1.1&gt;</description>
<packages>
<package name="TEST_MATE_TYPE_1">
</package>
<package name="TEST_MATE_TYPE_2">
</package>
<package name="TEST_MATE_TYPE_3">
</package>
</packages>
<symbols>
<symbol name="TEST_MATE_TYPE_1">
<pin name="BOARD_DETECT"/>
<pin name="ANA_IN101"/>
<pin name="ANA_IN102"/>
<pin name="ANA_IN103"/>
<pin name="ANA_IN104"/>
<pin name="ANA_OUT101"/>
<pin name="ANA_OUT102"/>
<pin name="ANA_OUT103"/>
<pin name="ANA_OUT104"/>
<pin name="DIG_IN101"/>
<pin name="DIG_IN102"/>
<pin name="DIG_IN103"/>
<pin name="DIG_IN104"/>
<pin name="DIG_OUT101.1"/>
<pin name="DIG_OUT101.2"/>
<pin name="DIG_OUT101.3"/>
<pin name="DIG_OUT101.4"/>
<pin name="SERIAL_101_TX"/>
<pin name="SERIAL_101_RX"/>
<pin name="SUPPLY101"/>
<pin name="GND"/>
</symbol>
<symbol name="TEST_MATE_TYPE_2">
<pin name="BOARD_DETECT"/>
<pin name="ANA_IN201"/>
<pin name="ANA_IN202"/>
<pin name="RS485_201_A"/>
<pin name="RS485_201_B"/>
<pin name="CAN_201_L"/>
<pin name="CAN_201_H"/>
<pin name="I2C_201_SDA"/>
<pin name="I2C_201_SCL"/>
<pin name="DIG_IN201"/>
<pin name="DIG_IN202"/>
<pin name="DIG_IN203"/>
<pin name="DIG_IN204"/>
<pin name="DIG_OUT201.1"/>
<pin name="DIG_OUT201.2"/>
<pin name="DIG_OUT201.3"/>
<pin name="DIG_OUT201.4"/>
<pin name="SERIAL_201_TX"/>
<pin name="SERIAL_201_RX"/>
<pin name="SUPPLY_201"/>
<pin name="GND"/>
<pin name="SERIAL_VCC"/>
</symbol>
<symbol name="TEST_MATE_TYPE_3">
<pin name="BOARD_DETECT"/>
<pin name="ANA_OUT301"/>
<pin name="ANA_OUT302"/>
<pin name="ANA_OUT303"/>
<pin name="ANA_OUT304"/>
<pin name="ANA/DIG_IN301"/>
<pin name="ANA/DIG_IN302"/>
<pin name="ANA/DIG_IN303"/>
<pin name="ANA/DIG_IN304"/>
<pin name="ANA/DIG_IN305"/>
<pin name="ANA/DIG_IN306"/>
<pin name="ANA/DIG_IN307"/>
<pin name="ANA/DIG_IN308"/>
<pin name="DIG_OUT301.2"/>
<pin name="DIG_OUT301.3"/>
<pin name="DIG_OUT301.4"/>
<pin name="DIG_OUT301.5"/>
<pin name="DIG_OUT301.6"/>
<pin name="DIG_OUT301.7"/>
<pin name="SUPPLY301"/>
<pin name="GND"/>
<pin name="DIG_OUT301.1"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="TEST_MATE_TYPE_1" prefix="TM">
<description>&lt;b&gt;TestMate Type 1 UUT footprint</description>
<gates>
<gate name="G$1" symbol="TEST_MATE_TYPE_1"/>
</gates>
<devices>
<device name="" package="TEST_MATE_TYPE_1">
<connects>
<connect gate="G$1" pin="ANA_IN101" pad="2"/>
<connect gate="G$1" pin="ANA_IN102" pad="3"/>
<connect gate="G$1" pin="ANA_IN103" pad="4"/>
<connect gate="G$1" pin="ANA_IN104" pad="5"/>
<connect gate="G$1" pin="ANA_OUT101" pad="6"/>
<connect gate="G$1" pin="ANA_OUT102" pad="7"/>
<connect gate="G$1" pin="ANA_OUT103" pad="8"/>
<connect gate="G$1" pin="ANA_OUT104" pad="9"/>
<connect gate="G$1" pin="BOARD_DETECT" pad="1"/>
<connect gate="G$1" pin="DIG_IN101" pad="10"/>
<connect gate="G$1" pin="DIG_IN102" pad="11"/>
<connect gate="G$1" pin="DIG_IN103" pad="12"/>
<connect gate="G$1" pin="DIG_IN104" pad="13"/>
<connect gate="G$1" pin="DIG_OUT101.1" pad="14"/>
<connect gate="G$1" pin="DIG_OUT101.2" pad="15"/>
<connect gate="G$1" pin="DIG_OUT101.3" pad="16"/>
<connect gate="G$1" pin="DIG_OUT101.4" pad="17"/>
<connect gate="G$1" pin="GND" pad="21"/>
<connect gate="G$1" pin="SERIAL_101_RX" pad="19"/>
<connect gate="G$1" pin="SERIAL_101_TX" pad="18"/>
<connect gate="G$1" pin="SUPPLY101" pad="20"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEST_MATE_TYPE_2" prefix="TM">
<description>&lt;b&gt;TestMate Type 2 UUT footprint</description>
<gates>
<gate name="G$1" symbol="TEST_MATE_TYPE_2"/>
</gates>
<devices>
<device name="" package="TEST_MATE_TYPE_2">
<connects>
<connect gate="G$1" pin="ANA_IN201" pad="2"/>
<connect gate="G$1" pin="ANA_IN202" pad="3"/>
<connect gate="G$1" pin="BOARD_DETECT" pad="1"/>
<connect gate="G$1" pin="CAN_201_H" pad="7"/>
<connect gate="G$1" pin="CAN_201_L" pad="6"/>
<connect gate="G$1" pin="DIG_IN201" pad="10"/>
<connect gate="G$1" pin="DIG_IN202" pad="11"/>
<connect gate="G$1" pin="DIG_IN203" pad="12"/>
<connect gate="G$1" pin="DIG_IN204" pad="13"/>
<connect gate="G$1" pin="DIG_OUT201.1" pad="15"/>
<connect gate="G$1" pin="DIG_OUT201.2" pad="16"/>
<connect gate="G$1" pin="DIG_OUT201.3" pad="17"/>
<connect gate="G$1" pin="DIG_OUT201.4" pad="18"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="I2C_201_SCL" pad="9"/>
<connect gate="G$1" pin="I2C_201_SDA" pad="8"/>
<connect gate="G$1" pin="RS485_201_A" pad="4"/>
<connect gate="G$1" pin="RS485_201_B" pad="5"/>
<connect gate="G$1" pin="SERIAL_201_RX" pad="20"/>
<connect gate="G$1" pin="SERIAL_201_TX" pad="19"/>
<connect gate="G$1" pin="SERIAL_VCC" pad="14"/>
<connect gate="G$1" pin="SUPPLY_201" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TEST_MATE_TYPE_3" prefix="TM">
<gates>
<gate name="G$1" symbol="TEST_MATE_TYPE_3"/>
</gates>
<devices>
<device name="" package="TEST_MATE_TYPE_3">
<connects>
<connect gate="G$1" pin="ANA/DIG_IN301" pad="6"/>
<connect gate="G$1" pin="ANA/DIG_IN302" pad="7"/>
<connect gate="G$1" pin="ANA/DIG_IN303" pad="8"/>
<connect gate="G$1" pin="ANA/DIG_IN304" pad="9"/>
<connect gate="G$1" pin="ANA/DIG_IN305" pad="10"/>
<connect gate="G$1" pin="ANA/DIG_IN306" pad="11"/>
<connect gate="G$1" pin="ANA/DIG_IN307" pad="12"/>
<connect gate="G$1" pin="ANA/DIG_IN308" pad="13"/>
<connect gate="G$1" pin="ANA_OUT301" pad="2"/>
<connect gate="G$1" pin="ANA_OUT302" pad="3"/>
<connect gate="G$1" pin="ANA_OUT303" pad="4"/>
<connect gate="G$1" pin="ANA_OUT304" pad="5"/>
<connect gate="G$1" pin="BOARD_DETECT" pad="1"/>
<connect gate="G$1" pin="DIG_OUT301.1" pad="14"/>
<connect gate="G$1" pin="DIG_OUT301.2" pad="15"/>
<connect gate="G$1" pin="DIG_OUT301.3" pad="16"/>
<connect gate="G$1" pin="DIG_OUT301.4" pad="17"/>
<connect gate="G$1" pin="DIG_OUT301.5" pad="18"/>
<connect gate="G$1" pin="DIG_OUT301.6" pad="19"/>
<connect gate="G$1" pin="DIG_OUT301.7" pad="20"/>
<connect gate="G$1" pin="GND" pad="22"/>
<connect gate="G$1" pin="SUPPLY301" pad="21"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
