| 14.5 |  | Task 3 - Configure IPSec Parameters |
| 14.5.6 |  | Task 4 - Applying the crypto map to an interface |

| Crypto maps are activated once applied to a specific interface of the PIX Security Appliance. It is necessary to thoroughly understand how IPSec traffic flows through the PIX Security Appliance so that a crypto map can be applied to the correct interface. Verify that access-lists applied to the same interface do not block ESP, AH, or ISAKMP traffic.

Use the following command to apply the crypto map to an interface :

> pix(config)# crypto map map-name interface interface-name

For example:

> crypto map mymap interface outside

| Lab Activity e-Lab Activity: Configure Crypto Map In this activity, the student will create a crypto map that will tie together an access-list and a transform set.