| 14.4 |  | Task 2 - Configure IKE Parameters |
| 14.4.4 |  | Step 4 - Verify IKE Phase 1 policies |

| The fourth step in configuring IKE parameters is to verify IKE phase one policies. The show isakmp policy command displays configured and default policies, as shown in Figure . The show isakmp command displays configured policies similar to the write terminal command output, as follows:

pix1(config)# show isakmp

isakmp enable outside

isakmp key ******** address 192.168.2.2 netmask 255.255.255.255

isakmp policy 10 authentication pre-share

isakmp policy 10 encryption des

isakmp policy 10 hash sha

isakmp policy 10 group 1

isakmp policy 10 lifetime 86400

| Lab Activity e-Lab Activity: Configure IKE Parameters In this activity, the student will demonstrate how to configure and verify IKE Phase 1 policy on the PIX Security Appliance.

| Lab Activity e-Lab Activity: Configure and Verify IKE Phase 1 Policy In this activity, the student will demonstrate how to configure and verify IKE Phase 1 policy on the PIX Security Appliance.